{"text_format":"1","workbook":"xlsx","n_sheets":20,"sheets":["Mainsheet","Completed","Calc","Areaofobs","Vessel_type","Deficiency_type","VIQrefno","Equipment_list","PSC_MOU","Inspection_type","Deficiency_Cause","Observer_code","Status_code","PSC_ref_no","Risk_value_of_obs","Year","Month","Date_","Sheet1","Ship_information"],"not_rendered":{"charts":0,"images":5,"macros":1,"external_links":0,"defined_names":12,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Mainsheet","index":0,"n_rows":44,"n_cols":28,"rows_kept":44,"cut":false,"hidden":false,"merged":[[10,8,10,9],[10,12,10,13],[12,6,12,27],[8,6,8,27]]}
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,"Defect - Damage Monitoring Sheet"]
[]
[null,null,null,null,null,null,null,"Date of Report","19-Dec-2019",null,null,"Ship Name","RESPECT (05-11-2019)"]
[]
[]
[]
[]
[]
[null,null,null,null,"ID","UNIQUE ID","Date Recorded","Type of Deficiency","Observer code","Type of Inspection","Description of Deficiency","Equipment Categories","Area of Observation","Deficiency Cause","VIQ Ref Number","Risk Value of Obs","PSC Ref Number","PSC MOU ID","Action Taken or Required","Target Date","PO Ref No.","Status Code","Date Completed","Drydock","Info Sharing","Critical Item","Audit Type","Superintendent Remarks"]
[null,null,null,null,4919,43766.276377314818,"2019-08-23","Observation","Ship Staff","Ship Staff Insp.","FO settling tank gauging is not working. Spares to be ordered and to be repaired when the settling tank is cleaned for IMO 2020 fuel","Aux. Mach.","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Waiting for spare","2019-12-22","RESP190152","Not Started",null,"No","No","No","Internal","RO under processing. "]
[null,null,null,null,4920,"24/10/2019 2:02:17 AM","2019-04-12","Deficiency","Ship Staff","Ship Staff Insp.","Echo Sounder log printing software \"FE800 Recording system\" unoperational.","Nav & comm. equip.","Navigation","Equipment Related",4.1900000000000004,"Low","Not Applicable","Not Applicable","Shore technician attendance required as per email from head office dated 24-Mar-2019.","2019-11-15",null,"In progress",null,"No","No","No","Internal","Capt.  Understand that you have been in discussion with Mr. Kumar of Navcom/IT Fleet with regads to same. Pls revert with update on same."]
[null,null,null,null,4921,"24/10/2019 3:58:43 AM","2019-04-25","Deficiency","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Cover of gears for all winches and windlass are in poor condition.Covers to be removed repaired and reinstalled after blasting and painting two coats of epoxy paint.","Mooring Mach.","Mooring","Equipment Related",9.14,"Medium","Not Applicable","Not Applicable","Cover gears of port and stbd winch fwd has been repaired and fitted back.","2020-03-15",null,"In progress",null,"No","No","No","Internal","Understand that crew started with de-rusting of port side windlass  cover. Pls advice current status based on percentage of work completed / still in progress."]
[null,null,null,null,4922,"24/10/2019 4:48:41 AM","2019-04-25","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Windlass and all winches to be fully blast and repaint with two coats of primer and one final coat red colour (same as deck colour) paint.","Mooring Mach.","Mooring","Equipment Related",9.14,"Medium","Not Applicable","Not Applicable","De-rusting of poop deck mooring winches in progress.","2020-03-20","RESP190062","In progress",null,"No","No","No","Internal","In VFF, this RO is Cancelled since Owner arranged supply & delivery direct to vessel. Pls advise if vessel have indeed received the paints onboard @ Cape Town on 18 Sep 2019. If yes, kindly revert with work progress."]
[null,null,null,null,4923,"24/10/2019 5:11:04 AM","2019-04-25","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Accommodation block front , port, stbd, and aft to be derusted and painted.","Accommodation ","General Appearance","External Factors",11.8,"Low","Not Applicable","Not Applicable","Derusting and painting of front completed. De-rusting of port and stbd bridge wing support pillars completed. De-rusting & painting of A-deck & B-deck port side completed.","2020-02-28","RESP190062","In progress",null,"No","No","No","Internal","In VFF, this RO is Cancelled since Owner arranged supply & delivery direct to vessel. Pls advise if vessel have indeed received the paints onboard @ Cape Town on 18 Sep 2019. If yes, kindly revert with work progress."]
[null,null,null,null,4924,"24/10/2019 5:31:51 PM","2019-04-25","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Upgrading maintenance on ballast tank to be carried out. 5P, 5S, 1P, 1S tank coating are in fair condition. For other tanks also some affected areas have to be upgraded before the special and CAP survey.","Hull & Tanks","Structural Condn. / WT integrity ","External Factors",2.8,"High","Not Applicable","Not Applicable","To be de-rusted nd painted.","2020-03-30","RESP190062","Not Started",null,"No","No","No","Internal","In VFF, this RO is Cancelled since Owner arranged supply & delivery direct to vessel. Pls advise if vessel have indeed received the paints onboard @ Cape Town on 18 Sep 2019. If yes, kindly revert with work progress."]
[null,null,null,null,4925,"24/10/2019 5:55:15 PM","2019-04-25","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Galley-Fridge not working. To be repaired or new one one to be procured.","Miscellaneous","MLC Related","Equipment Related",11.16,"Low","Not Applicable","Not Applicable","Awaiting for spare part manual to order reqd spares.","2020-01-30",null,"Not Started",null,"No","No","No","Internal","Spare parts manual obsolete as advised by maker. Details of compressor unit was provided to procurement  dept. (Mr. Sikander) on 06th Sept 2019, via email for obtaining of quotes."]
[null,null,null,null,4926,"24/10/2019 6:01:44 PM","2019-04-25","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Mooring Tails usage hrs have exceeded 18 months. To be replaced during next storing.","Miscellaneous","Mooring","Equipment Related",9.17,"High","Not Applicable","Not Applicable","Awaiting supply.","2020-01-31","RESP195064","Waiting spare",null,"No","No","No","Internal","Order currently at National Forwarders in Singapore, awaiting convenient port for supply."]
[null,null,null,null,4927,"24/10/2019 6:24:13 PM","2019-08-26","Observation","Ship Staff","Ship Staff Insp.","Fire bilge and ballast pump suction valve not holding.","Miscellaneous","Cargo / Ballast Systems","Equipment Related",10.31,"Very High","Not Applicable","Not Applicable","This valve requisition will be raised shortly.","2020-02-15",null,"Not Started",null,"Yes","No","No","Internal","Same to be included in dry-docking specification c/w details of the valve."]
[null,null,null,null,4928,"24/10/2019 6:29:35 PM","2019-08-23","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","The covers for the hydraulic boxes have damaged lips.","Deck Mach.","Cargo / Ballast Systems","External Factors",11.1,"High","Not Applicable","Not Applicable","same to be removed to engine room workshop and repaired and put back.","2020-03-31",null,"Not Started",null,"No","No","No","Internal","Noted that the job has yet to be started. Pls advice when you plan to commence same? "]
[null,null,null,null,4929,"24/10/2019 6:32:50 PM","2019-08-23","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Hospital door is damaged.","Accommodation ","General Appearance","External Factors",11.6,"Medium","Not Applicable","Not Applicable","Requisition will be raised in Jan'20 to get supply at Singapore.","2020-02-28",null,"Not Started",null,"No","No","No","Internal","Does the complete door needs replacing? \nPls issue & submit RO for supply of the door.                                                                                                                                                                                                                                                                                                                                                                                                                                                                          "]
[null,null,null,null,4930,"24/10/2019 6:47:57 PM","2019-08-23","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Paint is peeling of at several locations on main deck.","Deck Mach.","General Appearance","External Factors",11.1,"High","Not Applicable","Not Applicable","same be blasted/ buffed as found necessary and repainted.","2020-02-28",null,"In progress",null,"No","No","No","Internal","Pls revert with update on progress of the works, to date, based on percentage of job completed.                                                                                                                                                                                                                                                                                                                                                                                                                           "]
[null,null,null,null,4931,"24/10/2019 6:52:14 PM","2019-08-23","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","All rusted areas on main deck and poop deck to be spot blasted and painted with two coats of primer and one final coat of top.","Deck Mach.","General Appearance","External Factors",11.1,"High","Not Applicable","Not Applicable","All rusted areas on main deck and poop deck to be spot blasted and painted with two coats of primer and one final coat of top","2020-02-28",null,"In progress",null,"No","No","No","Internal","Pls revert with update on progress of the works, to date."]
[null,null,null,null,4932,"24/10/2019 6:56:25 PM","2019-08-23","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Pipe line supports and U clamps on deck are rusted.","Deck Pipe / Fittings","General Appearance","External Factors",11.5,"Medium","Not Applicable","Not Applicable","completed from fwd till no. 2C.O.T IG branch lines. The pipeline & associated supports from aft of manifold cross  deck lines till no.5 foam monitor completed. Painting of 2nd coat in progress from no.5 Foam monitor till P/V Breaker.","2020-02-22",null,"In progress",null,"No","No","No","Internal","Pls revert with update on progress of the work, to date."]
[null,null,null,null,4933,"24/10/2019 7:06:00 PM","2019-09-11","Observation","Ship Staff","Ship Staff Insp.","The port abd stbd side anchor hawse pipe cover has to be improved by fixing cross bars for better protection.","Miscellaneous","Structural Condn. / WT integrity ","Equipment Related",7.12,"High","Not Applicable","Not Applicable","The port abd stbd side anchor hawse pipe cover has to be improved by fixing cross bars for better protection.","2020-01-30",null,"Not Started",null,"No","No","No","Internal","Noted. Pls advice when you plan to commence said job."]
[null,null,null,null,4958,43766.279363425929,"2019-09-11","Observation","Ship Staff","Ship Staff Insp.","AC condenser sea water in andout valves are not holding","Miscellaneous","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Waiting for spare","2019-11-20","RESP190150","Not Started",null,"No","No","No","Internal","RO under processing."]
[null,null,null,null,4959,43766.280439814815,"2019-09-11","Observation","Ship Staff","Ship Staff Insp.","AE LO purifier speed sensor faulty","Purifier","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","waiting for spare","2019-11-20","RESP190110","Not Started",null,"No","No","No","Internal","Reference to VFF, RO was cancelled due to Owner arranging supply. Pls advice if you have received the requested spare part, supplied directly by Owner."]
[null,null,null,null,4960,43766.281631944446,"2019-09-25","Observation","Ship Staff","Ship Staff Insp.","No2 boiler feed water controller display malfunctioning","Boiler","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","...","2019-11-20",null,"Not Started",null,"No","No","No","Internal","Have investigation been carried out to verify possible cause of the mulfunction? If yes, pls revert with your findings c/w spares required. If not, when do you plan for same. "]
[null,null,null,null,4961,43766.282800925925,"2019-09-26","Observation","Ship Staff","Ship Staff Insp.","IG excess pressure controller not working","Inert Gas","Eng. / Strg. Comp.","Equipment Related",8.33,"Medium","Not Applicable","Not Applicable","fault found controller defective, same ordered","2019-11-20","RESP190167","Not Started",null,"No","No","No","Internal","RO under processing."]
[null,null,null,null,4962,43766.28398148148,"2019-10-13","Observation","Ship Staff","Ship Staff Insp.","Main engine unit #3 aft and unit #7 both outlet accumulator leaky","Main Engine ","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","waiting for spare","2019-11-30","RESP190170","Not Started",null,"No","No","No","Internal","Presume you have made temporary arrangements to control the leaks until requested spares are supplied. Will check with Procurement & advice status of the RO."]
[null,null,null,null,5840,43772.830034722225,"2019-10-15","Observation","Ship Staff","Ship Staff Insp.","Hydraulic oil leak in Steering gear compartment.","ER Pipes, valves & fittings","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","LEAK IS VERY MINOR BUT THE LOCATION OF PIPE IS S/G ROOM TOP BULKHEAD PROPER STAGING HAVE TO  RIGGED FOR ACCEBILITY ","2020-01-15",null,"Not Started",null,"No","No","No","Internal","Where is the location of leakage. What steps have been taken to minimise the leak until the suitable opportunity arises."]
[null,null,null,null,5841,43773.775358796294,"2019-10-15","Observation","Ship Staff","Ship Staff Insp.","one of the dresser coupling in bunker line leaky","Deck Pipe / Fittings","Eng. / Strg. Comp.","Equipment Related",8.41,"Medium","Not Applicable","Not Applicable","Dresser coupling tightened,spare ordered in store ","2020-01-15","RESP190113","Not Started",null,"No","No","No","Internal","Noted. Did you managed to stop the leak after tightening the coupling? RO is under processing. "]
[null,null,null,null,null,"20/12/2019 1:03:50 AM","2019-08-19","Deficiency","Owner / Marine / Tech. Suptd.","Suptd. Insp.","VDR Microphone & BNWAS reset button not available on bridge wings","Nav & comm. equip.","Navigation","Equipment Related",4.7,"High","Not Applicable","Not Applicable","Job Has been added in REFMAN for next scheduled Dry Dock.","2020-12-31",null,"Deferred to D D",null,"Yes",null,null,"Internal"]
[null,null,null,null,null,"20/12/2019 1:09:58 AM","2019-11-27","Observation","Ship Staff","Ship Staff Insp.","Hydraulic power pack oil cooler tube nest floating and cover found leaking.","Deck Mach.","Eng. / Strg. Comp.","Equipment Related",8.11,"Medium","Not Applicable","Not Applicable","O-Ring have to be changed.","2020-01-30",null,"Not Started",null,"No",null,null,"Internal"]
[null,null,null,null,null,"20/12/2019 1:17:15 AM","2019-08-21","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Missing / Poor condition of anti-skid paint coating at mooring area.","Mooring Mach.","Mooring","Inappropriate Procedure",11.3,"Medium","Not Applicable","Not Applicable","Vessel received Anti-skid paint on 05-Dec-19 and has already started de-rusting of Poop deck mooring area.","2019-12-31",null,"In progress",null,"No",null,null,"External"]
[null,null,null,null,null,"20/12/2019 12:01:06 PM","2019-08-28","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","3 of the 5 nos of SCBA face masks noted slightly opaque","LSA / FFA","LSA / FFA Appliances","Equipment Related",5.43,"High","Not Applicable","Not Applicable","Supply of face masks expected in Mid Jan 2020 when vessel calls Singapore","2020-01-30","RESP190136","Waiting spare",null,"No",null,null,"Internal"]
[null,null,null,null,null,"20/12/2019 12:07:54 PM","2019-08-29","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Fire Doors for the emergency exit in the E/R at the steering gear and at the bottom platform need renewal of fittings and door closers. (Doors not closing fully)\r\n5 nos of door around accommodation with door closers need renewal of door closers, 8 nos need adjustments .  Galley doors to the mess-rooms donot have door closers.","Accommodation ","Structural Condn. / WT integrity ","Equipment Related",11.14,"Medium","Not Applicable","Not Applicable","REQUISITION HAVE BEEN RAISED ABOUT THE DOOR LOCKING HANDLES HAVE BEEN MADE AND AWAITING SPARES.","2020-01-30","RESP190113","Waiting spare",null,"No",null,null,"Internal"]

{"sheet":"Completed","index":1,"n_rows":256,"n_cols":28,"rows_kept":256,"cut":false,"hidden":false,"merged":[[10,8,10,9],[10,12,10,13],[12,6,12,27],[8,6,8,27]]}
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,"Defect - Damage Monitoring Sheet"]
[]
[null,null,null,null,null,null,null,"Date of Report","19-11-2019",null,null,"Ship Name","RESPECT (05-11-2019)"]
[]
[]
[]
[]
[]
[null,null,null,null,"ID","UNIQUE ID","Date Recorded","Type of Deficiency","Observer code","Type of Inspection","Description of Deficiency","Equipment Categories","Area of Observation","Deficiency Cause","VIQ Ref Number","Risk Value of Obs","PSC Ref Number","PSC MOU ID","Action Taken or Required","Target Date","PO Ref No.","Status Code","Date Completed","Drydock","Info Sharing","Critical Item","Audit Type","Superintendent Remarks"]
[null,null,null,null,4938,"25/10/2019 7:19:54 PM","2019-05-08","Observation","Ship Staff","Ship Staff Insp.","BRIDGE WING DECK PAINT COATING CRACKED AND FLAKING OUT.","Hull & Tanks","General Appearance","External Factors","","","","","DECK TO BE CHIPPED AND HYDROBLASTED ,BUFFED ,TWO COATS OF PRIMER AND FINAL COAT TO BE APPLIED.","2019-05-30","","Completed","2019-05-29","No","No","No","Internal"]
[null,null,null,null,4939,"25/10/2019 7:21:58 PM","2019-04-25","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Before start of manoeuvring, after the engine is blow through, duty engineer to log in the E/R control log that the engine movements are given as per telegraph logger","Main Engine ","Eng. / Strg. Comp.","Equipment Related","","","","","Clear instruction given to duty engineer to log in the E/R Control log that the engine movements are given as per telegraph","2019-04-29","","Completed","2019-04-25","No","No","No","Internal"]
[null,null,null,null,4940,"25/10/2019 7:23:43 PM","2019-04-25","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Temp control xv/v for Pfr is leaking. To be rectified","Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Temp control xv/v for Pfr gland tightened and leak recified","2019-06-23","","Completed","2019-04-26","No","No","No","Internal"]
[null,null,null,null,4941,"25/10/2019 7:29:41 PM","2019-04-25","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Both vacuum pumps for Fire and Bilge p/p's, Vacuum p/p are seized.","Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Vacuum pump overhauled. Its in operation.","2019-06-01","","Completed","2019-06-01","No","No","No","Internal"]
[null,null,null,null,4942,"25/10/2019 7:31:48 PM","2019-04-25","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","The main air bottle auto drain valve was found shut. To be overhauled and put back in operation","Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Auto drain valve overhauled, put back in operation.","2019-05-11","","Completed","2019-07-02","No","No","No","Internal"]
[null,null,null,null,4943,"25/10/2019 7:42:49 PM","2019-04-25","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","The door closer of Funnel door is defective. To be repaired.","ER Pipes, valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","The door closer of Funnel door is repaired.","2019-05-11","","Completed","2019-05-10","No","No","No","Internal"]
[null,null,null,null,4944,"25/10/2019 7:44:26 PM","2019-04-25","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Electric starter panels are dirty, all of them are to be cleaned","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","Electric starter panels are cleaned.","2019-07-23","","Completed","2019-05-05","No","No","No","Internal"]
[null,null,null,null,4945,"25/10/2019 7:46:16 PM","2019-04-25","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Some lights were found not working in E/R casing. To be replaced.","ER Pipes, valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Lights were renewed.","2019-05-24","","Completed","2019-04-26","No","No","No","Internal"]
[null,null,null,null,4946,"25/10/2019 7:48:07 PM","2019-04-25","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Hot water leak on 3rd deck. To be rectified.","Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Leak rectified.","2019-06-23","","Completed","2019-05-25","No","No","No","Internal"]
[null,null,null,null,4947,"25/10/2019 7:50:49 PM","2019-05-07","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Hydrophore pump leaking","Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Gland packing tightened leak rectified","2019-06-20","","Completed","2019-06-08","No","No","No","Internal"]
[null,null,null,null,4948,"25/10/2019 7:52:23 PM","2019-05-07","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Emergency air bottle pressure was zero","Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Emergency air bottle filled and kept as standby","2019-05-20","","Completed","2019-05-09","No","No","No","Internal"]
[null,null,null,null,4949,"25/10/2019 7:58:38 PM","2019-05-07","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Jacket cooler SW pipe leaking","Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Jacket cooler SW pipe renewed","2019-05-31","","Completed","2019-05-23","No","No","No","Internal"]
[null,null,null,null,4950,"25/10/2019 8:00:07 PM","2019-05-07","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","....","Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","....","2019-05-31","","Completed","2019-05-23","No","No","No","Internal"]
[null,null,null,null,4951,"26/10/2019 5:13:55 AM","2019-05-08","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Notice near 15ppm should mention \"not to be operated without permission of Master and CE.","Aux. Engine","Eng. / Strg. Comp.","Inappropriate Procedure","","","","","New poster placed near OWS","2019-05-08","","Completed","2019-05-08","No","No","No","Internal"]
[null,null,null,null,4952,"26/10/2019 5:16:10 AM","2019-05-08","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Fire Bilge & ballast pump priming arrangement missing","Aux. Engine","Eng. / Strg. Comp.","Inappropriate Procedure","","","","","vacuum pump overhauled. Its in operation","2019-05-08","","Completed","2019-05-08","No","No","No","Internal"]
[null,null,null,null,4953,"26/10/2019 5:18:02 AM","2019-05-08","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Spring for DB tank sounding cap missing","Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","New spring put in place","2019-05-15","","Completed","2019-05-10","No","No","No","Internal"]
[null,null,null,null,4954,"26/10/2019 5:19:26 AM","2019-05-08","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Permanent RA for carrying out fuel v/v pressure test to be pasted neat the testing m/c recommended.","Main Engine ","Eng. / Strg. Comp.","Equipment Related","","","","","RA made and posted near testing m/c","2019-05-08","","Completed","2019-05-08","No","No","No","Internal"]
[null,null,null,null,4955,"26/10/2019 5:35:27 AM","2019-05-08","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ODME printer cartridge needs to be replaced.","Elect. Mach. & Equip.","Cargo / Ballast Systems","Equipment Related","","","","","ODME printer cartridge renewed.","2019-05-20","","Completed","2019-05-09","No","No","No","Internal"]
[null,null,null,null,4956,"26/10/2019 5:38:22 AM","2019-05-08","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Fwd air cooler SW inlet pipe leaking","Main Engine ","Eng. / Strg. Comp.","Equipment Related","","","","","Fwd air cooler SW inlet pipe leak rectified","2019-05-25","","Completed","2019-05-12","No","No","No","Internal"]
[null,null,null,null,4963,"23/10/2019 4:30:46 AM","2019-01-07","Deficiency","Ship Staff","Ship Staff Insp.","Main drain line of winch hydraulic system is holed.","Mooring Mach.","Mooring","Equipment Related","","","","","Hole repaired.","2019-01-15","","Completed","2019-01-10","No","No","No","Internal"]
[null,null,null,null,4964,"25/10/2019 1:46:40 AM","2019-01-11","Deficiency","Ship Staff","Ship Staff Insp.","Fresh water tanks vent head mess screen and their frames found in bad condition.","Deck Pipe / Fittings","Structural Condn. / WT integrity ","Equipment Related","","","","","Mess screen renewed and frames fabricated.","2019-01-14","","Completed","2019-01-11","No","No","No","Internal"]
[null,null,null,null,4965,"25/10/2019 1:51:42 AM","2019-01-08","Deficiency","Ship Staff","Ship Staff Insp.","Locking arrangement for toggle pin of harbour pin is broken.\t","LSA / FFA","LSA / FFA Appliances","Equipment Related","","","","","Locking arrangement fabricated.","2019-01-10","","Completed","2019-01-09","No","No","No","Internal"]
[null,null,null,null,4966,"25/10/2019 2:01:42 AM","2018-09-12","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Deck maintenance from Light post stbd fwd to MW2 to be derusted and painted,30% completed from last inspection.","Deck Pipe / Fittings","General Appearance","Equipment Related","","","","","Deck maintenance from Light post stbd fwd to MW2 to be derusted and full coat painted.","2019-01-31","","Completed","2019-01-28","No","No","No","Internal"]
[null,null,null,null,4967,"25/10/2019 2:09:14 AM","2018-12-11","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Snapback zone fwd and aft were not clearly visible due to recently painted deck.# Old snapback zone (sector shaped marking) to.","Hull & Tanks","General Appearance","Knowledge Based","","","","","Old snapback zone removed.","2019-03-31","","Completed","2019-01-19","No","No","No","Internal"]
[null,null,null,null,4968,"25/10/2019 2:12:49 AM","2018-12-15","Deficiency","Ship Staff","Ship Staff Insp.","Main Engine Unit #7 - FWD Fuel oil high pressure pipe found leaking from the union. Same to be replaced","Main Engine ","Eng. / Strg. Comp.","Equipment Related","","","","","HP pipe replaced with spare new pipe with adjusted distances as per maker's instructions","2018-12-18","","Completed","2019-12-18","No","No","No","Internal"]
[null,null,null,null,4969,"25/10/2019 2:18:00 AM","2019-01-05","Deficiency","Ship Staff","Ship Staff Insp.","EGE feed pump no.1 - found the FW inlet valve was not operational. Valve spindle found to be broken and valve seat stuck in the body.","ER Pipes, valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Valve replaced with new valve.","2019-01-18","","Completed","2019-01-15","No","No","No","Internal"]
[null,null,null,null,4970,"25/10/2019 2:22:47 AM","2019-01-10","Deficiency","Ship Staff","Ship Staff Insp.","Tank level float/bob of Waste Oil service tank no:2 was found defective","ER Pipes, valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Level gauge pulley wire was found stuck and same rectified. Made operational now","2019-01-16","","Completed","2019-01-15","No","No","No","Internal"]
[null,null,null,null,4971,"25/10/2019 2:26:19 AM","2019-01-15","Deficiency","Ship Staff","Ship Staff Insp.","Steam leaks on purifier heater seam inlet valves and boiler heating return lines to be rectified.","ER Pipes, valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Steam leaks attended and rectified.","2019-01-28","","Completed","2019-01-26","No","No","No","Internal"]
[null,null,null,null,4972,"25/10/2019 2:29:16 AM","2019-01-17","Deficiency","Ship Staff","Ship Staff Insp.","Hydrophore tank save all drain line found choked. Same to be cleared.","ER Pipes, valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Pipeline removed and choke rectified. Metal mesh fabricated and put in place.","2019-01-19","","Completed","2019-01-18","No","No","No","Internal"]
[null,null,null,null,4973,"25/10/2019 2:32:41 AM","2019-02-07","Deficiency","Ship Staff","Ship Staff Insp.","A few strands of fwd and aft lashing wire of port life boat were found broken.","LSA / FFA","LSA / FFA Appliances","Equipment Related","","","","","Lashing wire renewed.","2019-02-15","","Completed","2019-02-09","No","No","No","Internal"]
[null,null,null,null,4974,"25/10/2019 2:36:18 AM","2019-02-12","Deficiency","Ship Staff","Ship Staff Insp.","Vapour lines drain valves  found choked.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","Valves cleared and tried out","2019-02-15","","Completed","2019-02-13","No","No","No","Internal"]
[null,null,null,null,4975,"25/10/2019 2:39:12 AM","2019-01-25","Deficiency","Ship Staff","Ship Staff Insp.","AC blower unit drain line modification to be made","ER Pipes, valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Drain line cleared and line modified for ease of draining.","2019-02-28","","Completed","2019-02-06","No","No","No","Internal"]
[null,null,null,null,4976,"25/10/2019 2:41:29 AM","2019-01-25","Deficiency","Ship Staff","Ship Staff Insp.","Waste oil service tanks no:1 and 2- vent head flame arrestors to be checked and cleaned.","ER Pipes, valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Same checked and found normal","2019-02-15","","Completed","2019-02-07","No","No","No","Internal"]
[null,null,null,null,4977,"25/10/2019 2:43:42 AM","2019-01-28","Deficiency","Ship Staff","Ship Staff Insp.","Air regulator for control air found defective and not operational","ER Pipes, valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Air Regulator isolated and removed from place, Overhauled and put back. Same put in use now.","2019-02-15","","Completed","2019-02-06","No","No","No","Internal"]
[null,null,null,null,4978,"25/10/2019 2:49:16 AM","2019-01-30","Deficiency","Ship Staff","Ship Staff Insp.","ME Fuel Injector Testing machine found to be working inefficiently. Venting function and pressure tsting is found erratic.","Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Fuel Injector testing machine overhauled with the spares available onboard and same made operational.","2019-02-15","","Completed","2019-02-05","No","No","No","Internal"]
[null,null,null,null,4979,"25/10/2019 2:52:10 AM","2019-01-31","Deficiency","Ship Staff","Ship Staff Insp.","Drinking water hydrophore pump - Gland to be renewed and pump to be overhauled if necessary.","Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Pump overhauled and gland packing renewed. Pump operational now.","2019-02-15","","Completed","2019-02-05","No","No","No","Internal"]
[null,null,null,null,4980,"25/10/2019 2:54:00 AM","2019-02-14","Deficiency","Ship Staff","Ship Staff Insp.","Main Engine turbocharger differential pressure manometer for air filter not working. Same to be attended.","Main Engine ","Eng. / Strg. Comp.","Equipment Related","","","","","Manometer removed from place. Cleaned and filled with liquid and fitted back. Same working now.","2019-02-28","","Completed","2019-02-23","No","No","No","Internal"]
[null,null,null,null,4981,"25/10/2019 3:00:58 AM","2019-02-16","Deficiency","Ship Staff","Ship Staff Insp.","Mid-Ships STBD Hose handeling crane- Hydraulic oil leak to be investigated and rectified","Deck Mach.","Emgcy. Systems","Equipment Related","","","","","Upon investigation, found the seal on Hydraulic oil tank return filter leaking.Same changed with spare new return filter and seal ring.Crane tested found no leaks.","2019-02-28","","Completed","2019-02-22","No","No","No","Internal"]
[null,null,null,null,4982,"25/10/2019 3:05:33 AM","2018-09-12","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ER exhaust pipeline for Boiler and EGB and the insulation behind to be cleaned","ER Pipes, valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Pipelines and ductings cleaned and laggings renewed as necessary","2018-10-12","","Completed","2019-02-22","No","No","No","Internal"]
[null,null,null,null,4983,"25/10/2019 3:09:00 AM","2019-02-23","Deficiency","Ship Staff","Ship Staff Insp.","The Auto-drain water separator filter unit fitted on the service air line was found not working","ER Pipes, valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Unit removed, overhauled and assembled back. Same functional now.","2019-02-28","","Completed","2019-02-25","No","No","No","Internal"]
[null,null,null,null,4984,"25/10/2019 3:13:01 AM","2019-02-26","Deficiency","Ship Staff","Ship Staff Insp.","Aux.Boiler No.1 - One of the heating coil valve flange gasket steam leakage.","Deck Mach.","Emgcy. Systems","Equipment Related","","","","","Boiler isolated and gasket renewed with meta-flex gasket.","2019-02-26","","Completed","2019-02-26","No","No","No","Internal"]
[null,null,null,null,4985,"25/10/2019 3:19:29 AM","2019-02-25","Deficiency","Ship Staff","Ship Staff Insp.","One of the elbowconnections of hydrualic hoses was found leaking.","Deck Mach.","General Appearance","Equipment Related","","","","","Leak rectified after braising the connector,crane tried, no leakage observed.","2019-02-27","","Completed","2019-02-27","No","No","No","Internal"]
[null,null,null,null,4986,"25/10/2019 3:25:09 AM","2018-09-12","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","COW machines on deck and the isolation valve for the tanks 2,3,4,5, to be de rusted and painted.","Deck Pipe / Fittings","General Appearance","Equipment Related","","","","","De- rusting near COW branch lines for 1,,2,3,4 across completed,rest in progress.","2019-02-28","","Completed","2019-02-27","No","No","No","Internal"]
[null,null,null,null,4987,"25/10/2019 3:28:59 AM","2018-09-12","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Cow branch pipelines to be deruted and painted.","Deck Pipe / Fittings","General Appearance","Equipment Related","","","","","De-rusting near 1P,1S,2P,3P & 3S COT in progress","2019-01-31","","Completed","2019-02-27","No","No","No","Internal"]
[null,null,null,null,4988,"25/10/2019 3:33:50 AM","2018-08-09","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Heavy rust on main and return Hydraulic main line.","Deck Pipe / Fittings","General Appearance","Equipment Related","","","","","All mooring winches branch lines hydo blasted and leaking ones repaired.Pending is the main hydraulic line from fwd to aft.Planned to start the job after departure Long Beach.","2019-01-31","","Completed","2019-03-01","No","No","No","Internal"]
[null,null,null,null,4989,"25/10/2019 3:39:01 AM","2018-09-12","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Hydraulic valves for thr pump room,828 found small LO leakage from Actuators.To confirm the seal kit and attened.","Cargo Mach.","Emgcy. Systems","Equipment Related","","","","","Currently there is no leakage, valve operated and verified.","2019-03-31","","Completed","2019-03-11","No","No","No","Internal"]
[null,null,null,null,4990,"25/10/2019 4:41:30 AM","2019-03-06","Deficiency","Ship Staff","Ship Staff Insp.","Protective rail on STBD crane operator platform found broken and out of place.","Deck Mach.","Emgcy. Systems","Equipment Related","","","","","A new protective handle fabricated and put in place.","2019-03-15","","Completed","2019-03-10","No","No","No","Internal"]
[null,null,null,null,4991,"25/10/2019 5:21:23 AM","2018-09-18","Deficiency","Ship Staff","Ship Staff Insp.","IG pressure for 4 P,4 C & 1 S COT showing erroneous reading in CCR. Unable to reset pressure sensor.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","Two pressure gauages received at Singaporeon 5th Nov 18. Renewed the defective ones on 4 P & 4 S COT.Currently all cargo showing correct readings.","2018-12-15","NERI180229","Completed","2019-03-06","No","No","No","Internal"]
[null,null,null,null,4992,"25/10/2019 5:29:28 AM","2018-11-22","Deficiency","Ship Staff","Ship Staff Insp.","5 P COT PV valve leaking from suction side.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","Lapping and cleaningof seat carried out, No leak observed.","2018-12-15","NERI180260","Completed","2019-03-17","No","No","No","Internal"]
[null,null,null,null,4993,"25/10/2019 5:31:59 AM","2019-03-10","Deficiency","Ship Staff","Ship Staff Insp.","ME unit #5- HP Fuel pump's FWD high pressure pipe found leaking","Main Engine ","Eng. / Strg. Comp.","Equipment Related","","","","","HP pipe replaced with a spare new pipe","2019-03-15","","Completed","2019-03-12","No","No","No","Internal"]
[null,null,null,null,4994,"25/10/2019 5:57:55 AM","2019-03-15","Deficiency","Ship Staff","Ship Staff Insp.","ME #2 unit - Air starting valve found leaking","Main Engine ","Eng. / Strg. Comp.","Equipment Related","","","","","Same replace with a sapre overhauled valve","2019-03-20","","Completed","2019-03-16","No","No","No","Internal"]
[null,null,null,null,4995,"25/10/2019 6:26:26 AM","2018-12-11","Deficiency","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Vessel does not have any operational microwave in crew or officers pantry","Elect. Mach. & Equip.","Ice Opns.","Equipment Related","","","","","Vessel received 1 microwave during Singapore transit","2019-03-31","","Completed","2019-03-02","No","No","No","Internal"]
[null,null,null,null,4996,"25/10/2019 6:35:48 AM","2018-09-12","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","CO2 mushroom exhaust fan to be opened up and valve lied to be derusted and painted.  ","Deck Pipe / Fittings","General Appearance","Equipment Related","","","","","De- rusted and painted.","2019-02-28","","Completed","2019-03-17","No","No","No","Internal"]
[null,null,null,null,4997,"25/10/2019 6:40:02 AM","2019-02-18","Deficiency","Ship Staff","Ship Staff Insp.","Railings of the stowing platform of STBD crane jib is broken at 3 places.","Deck Mach.","General Appearance","Equipment Related","","","","","New railings were fabricated and put in place.","2019-03-31","","Completed","2019-03-18","No","No","No","Internal"]
[null,null,null,null,4998,"25/10/2019 6:41:45 AM","2019-02-12","Deficiency","Ship Staff","Ship Staff Insp.","Main Engine units #3 and #6 - Scavenge underpiston temperature high","Main Engine ","Eng. / Strg. Comp.","Equipment Related","","","","","During scavenge inspection done on 18/03/2019 found units 3 and 6 top piston rings broken. De-carb of same units carried out on 26/03/2019 and 22/03/2019 respectively.","2019-03-31","","Completed","2019-03-26","No","No","No","Internal"]
[null,null,null,null,4999,"25/10/2019 6:43:56 AM","2019-03-17","Deficiency","Ship Staff","Ship Staff Insp.","Air Con. condensor cooling SW return line pipe section leaking","ER Pipes, valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Pipe section removed. Found to be holed. Pipe section fabricated and same renewed","2019-04-15","","Completed","2019-04-02","No","No","No","Internal"]
[null,null,null,null,5000,"25/10/2019 6:45:52 AM","2019-03-18","Deficiency","Ship Staff","Ship Staff Insp.","ME unit #2 - Exhaust valve FW leak from bottom piece O-rings. Same to be renewed.","Main Engine ","Eng. / Strg. Comp.","Equipment Related","","","","","Exhaust valve pulled out and O-rings renewed and no FW leaks now.","2019-04-15","","Completed","2019-03-30","No","No","No","Internal"]
[null,null,null,null,5001,"25/10/2019 6:52:29 AM","2018-09-12","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Ballast tank Vent head maintenance for the spare Vent head kept on poop side of the deck to be carried out.Good condition vent head to be kept as spare and protected.","Miscellaneous","General Appearance","Inappropriate Procedure","","","","","All the vents kept on poop deck are heavily rusted.They are beyonds repairs as the de- rusting will increase the opening.","2019-01-31","","Completed","2019-03-31","No","No","No","Internal"]
[null,null,null,null,5002,"25/10/2019 6:58:28 AM","2019-03-16","Deficiency","Ship Staff","Ship Staff Insp.","Mooring winch no3 aft drum's brake handle is found defective.","Mooring Mach.","Emgcy. Systems","Equipment Related","","","","","Handle removed and locking plate fixed,put in place and tested.","2019-03-19","","Completed","2019-03-18","No","No","No","Internal"]
[null,null,null,null,5003,"25/10/2019 7:03:20 AM","2019-03-26","Deficiency","Ship Staff","Ship Staff Insp.","Jib stowing platform of both the hose handling crane does not have protective chains/rails.","Deck Mach.","Emgcy. Systems","Equipment Related","","","","","Chain arrangement made to secure the stowing platform.","2019-03-31","","Completed","2019-03-28","No","No","No","Internal"]
[null,null,null,null,5004,"25/10/2019 7:07:28 AM","2019-03-28","Deficiency","Ship Staff","Ship Staff Insp.","Air hose of STBD gangway shifting motor was found defective and leaking.","Deck Mach.","General Appearance","Equipment Related","","","","","Air hose replaced with the new one.","2019-03-31","","Completed","2019-03-29","No","No","No","Internal"]
[null,null,null,null,5005,"25/10/2019 7:13:53 AM","2018-10-03","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","MERCATOR name full paintaing on both side hull sides.\t\t\t","Hull & Tanks","General Appearance","External Factors","","","","","Vessel expecting name changed therefore paintaing will be carried out after the changes.","2018-12-30","","Completed","2019-04-01","No","No","No","Internal"]
[null,null,null,null,5006,"25/10/2019 7:17:34 AM","2018-09-12","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Stern View paint for the ship name and IMO No. to be painted.","Hull & Tanks","General Appearance","External Factors","","","","","vessel expecting name change therefore the job will be carried out after the change of name.","2019-01-31","","Completed","2019-04-01","No","No","No","Internal"]
[null,null,null,null,5007,"25/10/2019 7:19:18 AM","2019-04-01","Deficiency","Ship Staff","Ship Staff Insp.","Solenoid operated direction control valve no:40 for VIT actuator found leaking on Main Engine pneumatic control system","Main Engine ","Eng. / Strg. Comp.","Equipment Related","","","","","Same replaced with spare new valve and found satisfactory.","2019-04-15","","Completed","2019-04-03","No","No","No","Internal"]
[null,null,null,null,5008,"25/10/2019 7:47:37 AM","2019-03-31","Deficiency","Ship Staff","Ship Staff Insp.","U- clamps of life buoy's bracket on stbd side aft of the manifold is heavily rusted.","LSA / FFA","LSA / FFA Appliances","Equipment Related","","","","","New U- clamps to be put in place after removing the old ones.","2019-04-07","","Completed","2019-04-02","No","No","No","Internal"]
[null,null,null,null,5009,"25/10/2019 7:53:46 AM","2019-03-28","Observation","Ship Staff","Ship Staff Insp.","Floats of ballast vent heads of 3P Fwd, 3P Aft, 4P Fwd, 4S Aft were found to have slight crack in the body.","Miscellaneous","Cargo / Ballast Systems","Equipment Related","","","","","Replace with new ones.","2019-04-30","NERI190073","Completed","2019-04-11","No","No","No","Internal"]
[null,null,null,null,5010,"25/10/2019 7:58:35 AM","2018-11-26","Deficiency","Ship Staff","Ship Staff Insp.","Rudder angle indicator feedback linkage broken.","Hull & Tanks","Navigation","Equipment Related","","","","","same been welded and fixed,raised req for new one.","2019-01-15","NERI180300","Completed","2019-04-18","No","No","No","Internal"]
[null,null,null,null,5011,"25/10/2019 8:04:37 AM","2018-12-11","Deficiency","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Rudder angle indicator in wheel house displays 2 Deg PORT while rudder is midship. The error varies on port and starboard helm.Rudder angle indicator in wheel house displays 2 Deg PORT while rudder is midship. The error varies on port and starboard helm.","Nav & comm. equip.","Navigation","Equipment Related","","","","","Awaiting spares.","2019-03-31","NERI190014 and NERI190015","Completed","2019-04-18","No","No","No","Internal"]
[null,null,null,null,5012,"25/10/2019 8:07:21 AM","2018-12-11","Deficiency","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Transparent acrylic guard on engine lathe machine was found broken","ER Pipes, valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Face shield kept near the lathe for use","2019-03-31","","Completed","2019-04-18","No","No","No","Internal"]
[null,null,null,null,5013,"25/10/2019 8:09:31 AM","2019-02-20","Deficiency","Ship Staff","Ship Staff Insp.","AE inlet flowmeter not functioning","ER Pipes, valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Same replaced with new one","2019-04-30","","Completed","2019-04-20","No","No","No","Internal"]
[null,null,null,null,5014,"25/10/2019 8:12:02 AM","2019-02-28","Deficiency","Ship Staff","Ship Staff Insp.","....","Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","....","2019-04-30","","Completed","2019-04-18","No","No","No","Internal"]
[null,null,null,null,5015,"25/10/2019 8:14:09 AM","2019-02-28","Deficiency","Ship Staff","Ship Staff Insp.","Atmospheric condensor - not coping up. Tubes to be cleaned.","Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Condenser replaced with spare condenser","2019-04-30","","Completed","2019-04-18","No","No","No","Internal"]
[null,null,null,null,5016,"25/10/2019 8:15:54 AM","2019-04-05","Deficiency","Ship Staff","Ship Staff Insp.","Atmospheric condenser steam dumping valves leaks","Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","Overhauled reducing valve and isolation valve","2019-05-01","","Completed","2019-04-18","No","No","No","Internal"]
[null,null,null,null,5017,"25/10/2019 8:21:34 AM","2018-10-10","Deficiency","Ship Staff","Ship Staff Insp.","No 5 S COT PV valve leaking from pressure side.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","Overhauled twice. Still leaking. Need spare disc & as the present disc & seat are found with deep pits & highly corroded.","2018-12-30","NERI180260","Completed","2019-04-20","No","No","No","Internal"]
[null,null,null,null,5018,"25/10/2019 8:25:11 AM","2019-05-08","Deficiency","Ship Staff","Ship Staff Insp.","RESCUE STRETCHER IN PUMP ROOM STRAP BROKEN.","LSA / FFA","LSA / FFA Appliances","Equipment Related","","","","","SPARE STRETCHER RENEWED, BROKEN STRECHER REMOVED.","2019-05-10","","Completed","2019-05-08","No","No","No","Internal"]
[null,null,null,null,5019,"25/10/2019 8:30:03 AM","2019-05-08","Deficiency","Ship Staff","Ship Staff Insp.","RUBBER PACKING FOR WEATHERTIGHT DOORS OF CO2 ROOM AND FORECASTLE STORE FOUND CRACKED AND BROKEN.","Hull & Tanks","General Appearance","Equipment Related","","","","","RUBBER PACKING RENEWED.","2019-05-10","","Completed","2019-05-10","No","No","No","Internal"]
[null,null,null,null,5020,"25/10/2019 8:36:06 AM","2019-05-08","Observation","Ship Staff","Ship Staff Insp.","CHINA PASSAGE STOWED WITH GREASED BUCKETS, OLD PAINT DRUMS, WOODEN PALLETS, ROPES DIRECTLY BELLOW FUNNEL.","Miscellaneous","General Appearance","Human Error","","","","","OLD BUCKETS AND DRUMS CLEANED AND STORED IN LOCKER, WOODEN PALLETS AND ROPES STORED IN STEERING FLAT, CHINA PASSAGE CLEARED OF DEBRIS.","2019-05-11","","Completed","2019-05-11","No","No","No","Internal"]
[null,null,null,null,5021,"25/10/2019 9:01:20 AM","2019-04-25","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Some of the mesh for Ballast tank vent were found with incorrect size. All mesh to be checked and the ones which are big in size are to be replaced with correct size mesh.","Deck Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","","","","","All Ballast vent mesh renewed.","2019-05-05","","Completed","2019-04-26","No","No","No","Internal"]
[null,null,null,null,5022,"25/10/2019 5:33:38 PM","2019-04-25","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Some of the mesh for ballast tank ventwere found with incorrect size.All mesh to be checked and one which are big in size are to be replaced with correct size mesh.","Deck Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","","","","","All ballast vents mesh renewed.","2019-05-05","","Completed","2019-04-26","No","No","No","Internal"]
[null,null,null,null,5023,"25/10/2019 5:37:33 PM","2019-05-07","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ODME printer cartridge needs to be replaced.","Cargo Mach.","MARPOL Related","Equipment Related","","","","","ink ribbon renewed.","2019-05-10","","Completed","2019-05-09","No","No","No","Internal"]
[null,null,null,null,5024,"25/10/2019 5:45:12 PM","2019-05-07","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","pilot ladder should be in compliance with IMO resolution A.1045(27),please confirm the same.Attached message for reference.","Miscellaneous","General Appearance","Equipment Related","","","","","Vessel pilot ladder complying with IMO requirement.","2019-05-30","","Completed","2019-05-10","No","No","No","Internal"]
[null,null,null,null,5025,"25/10/2019 5:50:12 PM","2019-05-08","Deficiency","Ship Staff","Ship Staff Insp.","RUBBER PACKING FOR MUSHROOM VENTS FOUND BROKEN FOR SANITARY EXHAUST VENT ,STEERING FLAT VENTS.","LSA / FFA","LSA / FFA Appliances","Equipment Related","","","","","RUBBER PACKING RENEWED FOR COMPLETD SEALING ON CLOSURE.","2019-05-12","","Completed","2019-05-12","No","No","No","Internal"]
[null,null,null,null,5026,"25/10/2019 5:58:47 PM","2019-05-07","Deficiency","PSC Insp.","PSC Inspection","ENGINE ROOM BLOWER 1,2 AND 3 FLAPS NOT CLOSING COMPLETELY.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","Propulsion and auxiliary machinery",2,"HINGE HOLES BUILT UP DONE, SEAT BUILT UP DONE, BLOWER FLAPS 1,2 AND 3 SEALING 100%","2019-05-14","","Completed","2019-05-13","No","No","No","External"]
[null,null,null,null,5027,"25/10/2019 6:02:35 PM","2019-05-07","Deficiency","PSC Insp.","PSC Inspection","EMERGENCY GENERATOR DO TANK AIR VENT PIPE HOLED AND CORRODED BADLY","Deck Pipe / Fittings","Emgcy. Systems","Equipment Related","","","Emergency Systems",2,"FABRICATED A NEW AIR VENT PIPE AND REPLACED.","2019-05-14","","Completed","2019-05-14","No","No","No","External"]
[null,null,null,null,5028,"25/10/2019 6:07:23 PM","2019-05-13","Observation","Ship Staff","Ship Staff Insp.","AIR REGULATOR TO BE FIXED FOR CARGO SEACHEST EXXON TEST, PICTORIAL TEST, PROCEDURE TO BE PASTED NEAR CARGO SEACHEST VALVE.","Miscellaneous","Cargo / Ballast Systems","Equipment Related","","","","","AIR REGULATOR FIXED AND TEST PROCEDURES PASTED.","2019-05-30","","Completed","2019-05-15","No","No","No","Internal"]
[null,null,null,null,5029,"25/10/2019 6:16:06 PM","2019-05-09","Observation","Ship Staff","Ship Staff Insp.","PV Breaker to be de-rusted and painted, Check for calibration.","Inert Gas","Cargo / Ballast Systems","Equipment Related","","","","","PV Breaker de-rusted, inspected, liquid checked, full final coat painted, stencilled.","2019-06-30","","Completed","2019-05-17","No","No","No","Internal"]
[null,null,null,null,5030,"25/10/2019 6:18:58 PM","2019-04-25","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","COW machines to be de-rusted and painted.","Cargo Mach.","General Appearance","Equipment Related","","","","","COW machine valves greased and freed.","2019-05-20","","Completed","2019-05-18","No","No","No","Internal"]
[null,null,null,null,5031,"25/10/2019 6:22:41 PM","2019-04-25","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","All areas where primer has been applied to be washed and repainted at the earliest as recoating interval is only 15 days.","Hull & Tanks","General Appearance","Inappropriate Procedure","","","","","All primered areas throughly washed and painted.","2019-05-20","","Completed","2019-05-20","No","No","No","Internal"]
[null,null,null,null,5032,"25/10/2019 6:25:43 PM","2019-05-09","Deficiency","Ship Staff","Ship Staff Insp.","2C, 5C COT and 2s COT PV valve pressure side leaking.","Inert Gas","Cargo / Ballast Systems","Equipment Related","","","","","PV valves for 2C, 5C and 2S COT lapped and rectified, spare PV valve lapped and kept ready for emergency.","2019-05-30","","Completed","2019-05-21","No","No","No","Internal"]
[null,null,null,null,5033,"25/10/2019 6:28:39 PM","2019-04-25","Deficiency","Ship Staff","Ship Staff Insp.","No.2S COT PV valve leaking from pressure side.","Inert Gas","Cargo / Ballast Systems","Equipment Related","","","","","Overhauled, lapped the pressure seat and rectified.","2019-07-25","NERI190091","Completed","2019-05-21","No","No","No","Internal"]
[null,null,null,null,5034,"25/10/2019 6:43:20 PM","2019-04-25","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","COW line and fire line valves on deck found frozen. All these valves to be made free.","Deck Mach.","Cargo / Ballast Systems","Equipment Related","","","","","All COW and fire line valves made free, operable by hande.","2019-05-19","","Completed","2019-05-19","No","No","No","Internal"]
[null,null,null,null,5035,"25/10/2019 7:08:20 PM","2019-05-16","Observation","Ship Staff","Ship Staff Insp.","AIR HOSE FOR PORT SIDE PILOT LADDER SHIFTING REEL CRACKED AND BROKEN.","Miscellaneous","LSA / FFA Appliances","Equipment Related","","","","","AIR HOSE REPLASED.","2019-05-30","","Completed","2019-05-24","No","No","No","Internal"]
[null,null,null,null,5036,"25/10/2019 7:15:31 PM","2019-05-09","Observation","Ship Staff","Ship Staff Insp.","ALL COT PV VALVES NEED DERUSTING AND PAINTING.","Inert Gas","Cargo / Ballast Systems","Equipment Related","","","","","PV VALVES PIPES AND STAND DERUSTING AND PAINTING IN PROGRESS.","2019-06-30","","Completed","2019-05-30","No","No","No","Internal"]
[null,null,null,null,5037,"26/10/2019 5:40:12 AM","2019-05-08","Observation","Ship Staff","Ship Staff Insp.","pneumatic driven pump for AE not operational","Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Pump and air motor overhauled","2019-05-25","","Completed","2019-05-17","No","No","No","Internal"]
[null,null,null,null,5038,"26/10/2019 5:45:43 AM","2019-05-09","Observation","Ship Staff","Ship Staff Insp.","Emergency generator exhaust pipe badly corroded.","LSA / FFA","LSA / FFA Appliances","Equipment Related","","","","","Vent pipe renewed.","2019-06-15","","Completed","2019-05-14","No","No","No","Internal"]
[null,null,null,null,5039,"26/10/2019 5:42:12 AM","2019-05-09","Observation","Ship Staff","Ship Staff Insp.","Main cooling SW pump no.2 mech seal leaking","Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","main SW cooling pipe cleaned, no leak from seal","2019-06-15","","Completed","2019-05-27","No","No","No","Internal"]
[null,null,null,null,5040,"26/10/2019 5:51:45 AM","2019-05-09","Observation","Ship Staff","Ship Staff Insp.","Laggine at many places to be ratched up properly","Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Lagging renewed.","2019-06-15","","Completed","2019-05-27","No","No","No","Internal"]
[null,null,null,null,5041,"26/10/2019 5:49:26 AM","2019-05-09","Observation","Ship Staff","Ship Staff Insp.","EGB feed pump no.2 bearings need to be replaced.","Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Bearing renewed","2019-06-15","","Completed","2019-05-21","No","No","No","Internal"]
[null,null,null,null,5042,"26/10/2019 5:53:28 AM","2019-05-21","Observation","Ship Staff","Ship Staff Insp.","Drinking water pump leaking","Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Pump overhauled","2019-05-25","","Completed","2019-05-23","No","No","No","Internal"]
[null,null,null,null,5043,"26/10/2019 5:55:14 AM","2019-05-29","Observation","Ship Staff","Ship Staff Insp.","No2 waste oil tank sounding float not working","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","Float wire renewed","2019-06-15","","Completed","2019-05-29","No","No","No","Internal"]
[null,null,null,null,5044,"26/10/2019 6:00:42 AM","2018-08-09","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Toilet flush lever damaged in 4th engineer and master's cabin.","Accommodation ","MLC Related","Equipment Related","","","","","Toilet flush lever renewed in 4th engineer and maste's cabin.","2018-11-08","","Completed","2019-05-20","No","No","No","Internal"]
[null,null,null,null,5045,"26/10/2019 6:03:07 AM","2019-05-01","Observation","Ship Staff","Ship Staff Insp.","Fuel oil auto backwash filter elemens choked cannot be cleaned. Auto backwash filter not in use","ER Pipes, valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","New elements put in use, fuel oil backwash filter working.","2019-05-01","","Completed","2019-05-10","No","No","No","Internal"]
[null,null,null,null,5046,"26/10/2019 6:04:50 AM","2019-05-09","Observation","Ship Staff","Ship Staff Insp.","Main engine unit #5 indicator valve leak","Main Engine ","Eng. / Strg. Comp.","Equipment Related","","","","","Main engine unit #5 indicator valve renewed","2019-06-15","","Completed","2019-05-30","No","No","No","Internal"]
[null,null,null,null,5047,"26/10/2019 6:24:10 AM","2018-09-12","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","No.2 & 3 COP pneumatic discharged valve not functional remotely need to attend in emergency.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","Opened and inspected. Repaired carried out, Operational.","2018-10-12","NERI180282","Completed","2019-05-18","No","No","No","Internal"]
[null,null,null,null,5048,"26/10/2019 6:27:13 AM","2018-12-11","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Removed after installation of new (Wartsila) O2 analyser.","Inert Gas","Cargo / Ballast Systems","Equipment Related","","","","","Removed.","2019-03-31","","Completed","2019-05-19","No","No","No","Internal"]
[null,null,null,null,5049,"26/10/2019 6:36:22 AM","2018-12-11","Deficiency","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Was noticed when foam pump in standby mode.","LSA / FFA","LSA / FFA Appliances","Equipment Related","","","","","Rectified.","2019-03-31","","Completed","2019-05-25","No","No","No","Internal"]
[null,null,null,null,5050,"26/10/2019 6:40:51 AM","2018-12-11","Deficiency","Owner / Marine / Tech. Suptd.","Suptd. Insp.","AUS (Auto unloading system )in CCR is not operational.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","Troubleshoouting carried out, AUTOMATION to be checked, rectified.","2019-07-31","","Completed","2019-05-18","No","No","No","Internal"]
[null,null,null,null,5051,"26/10/2019 6:45:24 AM","2019-04-25","Deficiency","Ship Staff","Ship Staff Insp.","No 1 GPS stoped responding and not showing dispaly after replacement of internal battery by service engineer during annual at Qinhuangdao.","Nav & comm. equip.","Navigation","Equipment Related","","","","","New unit installed in Singapore,on 6th may 2019.","2019-05-08","","Completed","2019-05-06","No","No","No","Internal"]
[null,null,null,null,5052,"26/10/2019 6:49:44 AM","2019-04-25","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Hydro blaster motor is in poor condition.Maintenance to be carried out on the same and stored properly and properly covering with conwase.","Hull & Tanks","Structural Condn. / WT integrity ","Equipment Related","","","","","Maintenance carried out.","2019-05-20","","Completed","2019-05-18","No","No","No","Internal"]
[null,null,null,null,5053,"26/10/2019 6:59:51 AM","2019-04-25","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Galley - Potato peeler not working.To be repaired.","Miscellaneous","MLC Related","Equipment Related","","","","","Repaired.","2019-05-20","","Completed","2019-05-15","No","No","No","Internal"]
[null,null,null,null,5054,"26/10/2019 7:03:58 AM","2019-04-25","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Galley- Mixer not woking.To be repaired.","Miscellaneous","General Appearance","Equipment Related","","","","","Repaired.","2019-05-20","","Completed","2019-05-15","No","No","No","Internal"]
[null,null,null,null,5055,"26/10/2019 7:10:25 AM","2019-04-25","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Condition of cabin toilate to be improved.Many shower have been found leaking.Same to be rectified/renewed as necessary. Some flush in crew cabin has been reported as not working. Same to be rectified.","Accommodation ","MLC Related","Equipment Related","","","","","Cleaning carried out.Leaking shower head replaced.","2019-06-15","","Completed","2019-05-15","No","No","No","Internal"]
[null,null,null,null,5056,"25/10/2019 7:12:22 PM","2019-04-25","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Mattresses in some cabins are in poor condition. same to renewed.","Accommodation ","General Appearance","Human Error","","","","","Mattresses renewed.","2019-07-30","","Completed","2019-05-28","No","No","No","Internal"]
[null,null,null,null,5057,"26/10/2019 7:22:19 AM","2019-05-07","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","STBD side conduit pipe near LB, electrical wire pocket needs to be filled with electrical putty.","Miscellaneous","Emgcy. Systems","Equipment Related","","","","","Done","2019-05-30","","Completed","2019-05-25","No","No","No","Internal"]
[null,null,null,null,5058,"26/10/2019 7:27:15 AM","2019-04-25","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Boiler feed pump No.1 has been reported to be in poor condition.Spares to be supplied and same to.","Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Wating for spare.","2019-06-23","RESP195028","Completed","2019-05-28","No","No","No","Internal"]
[null,null,null,null,5059,"26/10/2019 7:30:07 AM","2019-04-25","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","AE LO attached p/p'sdue for overhaul. Spares to be ordered and pumps overhauled","Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Waiting for spare","2019-06-23","NERI190033","Completed","2019-05-20","No","No","No","Internal"]
[null,null,null,null,5060,"26/10/2019 8:32:25 AM","2019-01-24","Deficiency","Ship Staff","Ship Staff Insp.","Aft motor of port windlass is leakinf from shaft seal.","Mooring Mach.","Mooring","Equipment Related","","","","","Tested, Found no leak. Shall observe during next operation.","2019-04-30","","Completed","2019-04-30","No","No","No","Internal"]
[null,null,null,null,5061,"26/10/2019 8:34:24 AM","2019-02-28","Deficiency","Ship Staff","Ship Staff Insp.","Main Engine- Main air starting valve service limit switch broken and defective","Main Engine ","Eng. / Strg. Comp.","Equipment Related","","","","","Repairs carried out.","2019-08-30","","Completed","2019-05-30","No","No","No","Internal"]
[null,null,null,null,5062,"26/10/2019 8:40:56 AM","2019-04-25","Deficiency","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Leak on port windlass motor shaft seal.Seal to renew. Job to be undertaken in the ballast.","Mooring Mach.","Mooring","Equipment Related","","","","","Tested.Found no leak.Shall observe during next ops.","2019-05-30","","Completed","2019-05-30","No","No","No","Internal"]
[null,null,null,null,5063,"26/10/2019 9:14:35 AM","2018-09-12","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Stbd Drain pipe from bridge wing to FAN supply duct,2 angle bars rusted causing rust stains to be cleaned and painted china passage, Stbd side next ER ventilation opening one weld seem to be derusted.","Deck Pipe / Fittings","General Appearance","Equipment Related","","","","","Derusted and Painted.","2019-06-30","","Completed","2019-06-15","No","No","No","Internal"]
[null,null,null,null,5064,"27/10/2019 2:06:31 AM","2018-09-12","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Stbd bridge wing bottom i.e.D deck, derust and pain.","Accommodation ","General Appearance","External Factors","","","","","Derusted and Painted.","2019-06-30","","Completed","2019-06-15","No","No","No","Internal"]
[null,null,null,null,5065,"27/10/2019 2:10:56 AM","2019-04-25","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","AUS not working.To be recalibrated.Water was found in control system.Efficiency of control air dryer to be checked.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","AUS automation and valve operations repaired and tried out.","2019-05-20","","Completed","2019-05-18","No","No","No","Internal"]
[null,null,null,null,5066,"27/10/2019 2:14:20 AM","2019-05-09","Observation","Ship Staff","Ship Staff Insp.","Mast Riser derusting and paintaing to be done.","Inert Gas","Cargo / Ballast Systems","Equipment Related","","","","","Mast Riser derusted and painted full coat.","2019-08-09","","Completed","2019-06-10","No","No","No","Internal"]
[null,null,null,null,5067,"27/10/2019 2:25:51 AM","2019-05-09","Observation","Ship Staff","Ship Staff Insp.","Old man roller for SBM chain forecastle frozen, need to be freed.","Miscellaneous","Mooring","Equipment Related","","","","","Freed, greased Dismantled.","2019-08-09","","Completed","2019-06-14","No","No","No","Internal"]
[null,null,null,null,5068,"27/10/2019 2:34:13 AM","2019-05-12","Observation","Ship Staff","Ship Staff Insp.","Bridge doors not gas tight.","Miscellaneous","Navigation","External Factors","","","","","Rollers adjusted for proper sealing against rubber packing.","2019-08-12","","Completed","2019-06-06","No","No","No","Internal"]
[null,null,null,null,5069,"27/10/2019 2:42:06 AM","2018-12-11","Deficiency","Owner / Marine / Tech. Suptd.","Suptd. Insp.","No. 1 COP leakage from bottom seal.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","Bottom seal renewed.","2019-06-30","","Completed","2019-06-05","No","No","No","Internal"]
[null,null,null,null,5070,"27/10/2019 2:48:41 AM","2019-04-25","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Galley- A/C not working. To be repaired. Spares to be ordered.","Miscellaneous","MLC Related","Equipment Related","","","","","Repaired working fine.","2019-06-20","","Completed","2019-06-14","No","No","No","Internal"]
[null,null,null,null,5071,"27/10/2019 2:51:21 AM","2019-05-07","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Port side bunker high level alarm electrical pipe support bar wasted, needs renewal.","Miscellaneous","General Appearance","External Factors","","","","","renewed","2019-08-08","","Completed","2019-06-15","No","No","No","Internal"]
[null,null,null,null,5072,"27/10/2019 2:39:05 AM","2019-05-20","Deficiency","Ship Staff","Ship Staff Insp.","Scupper pipes on deck to be derusted and painted, Scupper plugs maintenance, Greasing and numbering to be carried.","Hull & Tanks","Structural Condn. / WT integrity ","Equipment Related","","","","","Scupper plugs and Scupper pipes derusted and maintenance carried out.","2019-08-20","","Completed","2019-06-15","No","No","No","Internal"]
[null,null,null,null,5073,"27/10/2019 3:23:25 AM","2019-05-07","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Electrical wire support bar for emg lighting near LB launching proceduers wasted, needs renewal.","Miscellaneous","General Appearance","External Factors","","","","","Renewed","2019-08-08","","Completed","2019-06-15","No","No","No","Internal"]
[null,null,null,null,5074,"27/10/2019 3:25:51 AM","2019-05-08","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","STBD side conduit pipe nar LB, electrical wire pocket needs to be filled with electrical putty.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","Renewed","2019-08-08","","Completed","2019-06-15","No","No","No","Internal"]
[null,null,null,null,5075,"27/10/2019 3:28:47 AM","2019-02-28","Deficiency","Ship Staff","Ship Staff Insp.","Hot well top covers and top plate corroded and leaking","Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","Top plate de rusted and painted","2019-06-15","","Completed","2019-06-02","No","No","No","Internal"]
[null,null,null,null,5076,"27/10/2019 3:30:40 AM","2019-05-10","Observation","Ship Staff","Ship Staff Insp.","Boiler water circulating pump discharge valve to no.1 BLR not holding","Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","Same valve renewed with new spare valves","2019-06-30","","Completed","2019-06-24","No","No","No","Internal"]
[null,null,null,null,5077,"27/10/2019 3:33:52 AM","2019-06-15","Observation","Ship Staff","Ship Staff Insp.","Galley A/C blower casing damaged.","Aux. Mach.","General Appearance","Equipment Related","","","","","Rectified","2019-08-08","","Completed","2019-06-24","No","No","No","Internal"]
[null,null,null,null,5078,"27/10/2019 3:55:37 AM","2019-06-16","Observation","Ship Staff","Ship Staff Insp.","Main SW pump no.1 mechanical seal leaky","Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Mechanical seal renewed","2019-08-08","","Completed","2019-06-19","No","No","No","Internal"]
[null,null,null,null,5079,"27/10/2019 3:57:38 AM","2019-05-09","Observation","Ship Staff","Ship Staff Insp.","Main SW upmp no.1 motor bearings to renewed as its making noise","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","Bearing renewed","2019-08-08","","Completed","2019-06-19","No","No","No","Internal"]
[null,null,null,null,5080,"27/10/2019 4:00:33 AM","2019-05-09","Observation","Ship Staff","Ship Staff Insp.","FWG/ Deck seal pump cover broken","Aux. Mach.","","Equipment Related","","","","","Await spares/ Broken cover fabricated","2019-08-08","RESP195061","Completed","2019-06-16","No","No","No","Internal"]
[null,null,null,null,5081,"27/10/2019 4:02:35 AM","2019-06-16","Observation","Ship Staff","Ship Staff Insp.","ME turbocharger grit washing pipe found choked","Main Engine ","Eng. / Strg. Comp.","Equipment Related","","","","","Same rectified","2019-06-30","","Completed","2019-06-21","No","No","No","Internal"]
[null,null,null,null,5082,"27/10/2019 4:04:19 AM","2019-06-17","Observation","Ship Staff","Ship Staff Insp.","AE No.2 unit #2 exhaust temperature high","Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","unit #2 FO pump renewed","2019-06-30","","Completed","2019-06-19","No","No","No","Internal"]
[null,null,null,null,5083,"27/10/2019 4:05:35 AM","2019-05-09","Observation","Ship Staff","Ship Staff Insp.","AE #1 Starting air pressure regulating valve found faulty","Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Same renewed with overhauled spare","2019-06-16","","Completed","2019-06-15","No","No","No","Internal"]
[null,null,null,null,5084,"27/10/2019 4:11:27 AM","2019-04-25","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Cargo Pressure monitoring system alarms in CCR is not working. To be rectified.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","Cargo pressur monitoring system in CCR checked,Alarm module is inactive in softwear, Unable to activate by ship staff.","2019-08-20","","Completed","2019-06-16","No","No","No","Internal"]
[null,null,null,null,5085,"27/10/2019 4:13:39 AM","2019-04-25","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","AC for the MSB room is not working. To be repaired on priority","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","Repaired carried out. Working satisfactorily","2019-07-25","","Completed","2019-06-16","No","No","No","Internal"]
[null,null,null,null,5086,"27/10/2019 4:17:06 AM","2019-06-26","Observation","Ship Staff","Ship Staff Insp.","Steam leak near FWG","Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","rectified","2019-06-30","","Completed","2019-06-26","No","No","No","Internal"]
[null,null,null,null,5087,"27/10/2019 4:29:12 AM","2019-06-25","Observation","Ship Staff","Ship Staff Insp.","Steam leak near incinerator","Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","rectified","2019-06-30","","Completed","2019-06-26","No","No","No","Internal"]
[null,null,null,null,5088,"27/10/2019 4:48:14 AM","2018-10-24","Deficiency","Ship Staff","Ship Staff Insp.","No. 2 COP AUS tank level transimtter requires calibration.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","Calibration carried out.","2019-08-15","","Completed","2019-06-20","No","No","No","Internal"]
[null,null,null,null,5089,"27/10/2019 4:51:55 AM","2018-11-14","Deficiency","Ship Staff","Ship Staff Insp.","Cargo educator discharge pressure transmitter defective.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","Line cleared, rectified.","2019-08-15","","Completed","2019-06-20","No","No","No","Internal"]
[null,null,null,null,5090,"27/10/2019 5:09:10 AM","2018-11-14","Deficiency","Ship Staff","Ship Staff Insp.","No.3 COP discharged pressure pneumatic transmitter in PR defective.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","Line cleared,rectified","2019-08-15","","Completed","2019-06-20","No","No","No","Internal"]
[null,null,null,null,5091,"27/10/2019 5:13:12 AM","2018-11-30","Deficiency","Ship Staff","Ship Staff Insp.","No.1 COP discharge & suction local pressure gauge in PR defective.It was compared during line pressure testing.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","Line cleared,rectified.","2019-08-15","","Completed","2019-06-20","No","No","No","Internal"]
[null,null,null,null,5092,"27/10/2019 5:19:24 AM","2018-12-11","Deficiency","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Following pressure gauge were found erratic.a) No.3 COP Discharge local and CCR panel gauge, b) Cargo eductor discharge gauge, c) No. 1 COP Suction & discharge gauge(Local).","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","Line cleared, rectified.","2019-08-15","","Completed","2019-06-20","No","No","No","Internal"]
[null,null,null,null,5093,"27/10/2019 5:24:08 AM","2019-04-25","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","In many areas old paint is peeling off on main deck.These section to be blasted and repainted.Vessel to start using the girt blaster and hydro.","Hull & Tanks","Structural Condn. / WT integrity ","Equipment Related","","","","","Hydroblasting completed.","2019-06-25","","Completed","2019-06-18","No","No","No","Internal"]
[null,null,null,null,5094,"27/10/2019 5:30:25 AM","2019-04-25","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Rusted area below the pipeline to be attended.This job to be put on priority now.Area to be blasted and coated with two coats of primer and one coat of polyurthane paint.","Hull & Tanks","Structural Condn. / WT integrity ","Equipment Related","","","","","Hydroblasting completed.","2019-06-25","","Completed","2019-06-18","No","No","No","Internal"]
[null,null,null,null,5095,"27/10/2019 5:33:12 AM","2019-05-09","Observation","Ship Staff","Ship Staff Insp.","Fridge compressor sump oil for both compressor needs to be changed","Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","oil renewed","2019-08-08","","Completed","2019-07-01","No","No","No","Internal"]
[null,null,null,null,5096,"27/10/2019 5:34:30 AM","2019-07-01","Observation","Ship Staff","Ship Staff Insp.","Oil leaking from AE F.O. duplex filter changing lever","Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","O ring renewed","2019-07-03","","Completed","2019-07-02","No","No","No","Internal"]
[null,null,null,null,5097,"27/10/2019 5:36:19 AM","2019-07-03","Observation","Ship Staff","Ship Staff Insp.","AE1 FO inlet valve bonnet leaky","Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Bonnet gasket renewed","2019-07-03","","Completed","2019-07-03","No","No","No","Internal"]
[null,null,null,null,5098,"27/10/2019 6:29:27 AM","2019-07-03","Observation","Ship Staff","Ship Staff Insp.","Incinerator service tank's drain choked","Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Tank to be cleaned","2019-07-15","","Completed","2019-07-06","No","No","No","Internal"]
[null,null,null,null,5099,"27/10/2019 6:30:57 AM","2019-07-05","Observation","Ship Staff","Ship Staff Insp.","ME LO purifier inlet temperature not rising","Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","To be cleaned","2019-07-06","","Completed","2019-07-06","No","No","No","Internal"]
[null,null,null,null,5100,"27/10/2019 6:33:06 AM","2019-07-03","Observation","Ship Staff","Ship Staff Insp.","Upper deck and mess room's drinking water fountain not working. Filter to be cleaned","Aux. Mach.","MLC Related","Equipment Related","","","","","Fountain working and filter cleaned","2019-07-10","","Completed","2019-07-05","No","No","No","Internal"]
[null,null,null,null,5101,"27/10/2019 6:37:50 AM","2019-05-09","Observation","Ship Staff","Ship Staff Insp.","Aux boiler DP transmitter valves not holding","Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","valves renewed","2019-08-08","","Completed","2019-07-16","No","No","No","Internal"]
[null,null,null,null,5102,"27/10/2019 6:40:38 AM","2019-04-25","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Engine casing area is dirty - To be cleaned","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","Cleaning and Painting done","2019-08-30","","Completed","2019-07-16","No","No","No","Internal"]
[null,null,null,null,5103,"27/10/2019 6:45:48 AM","2019-04-25","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Port side crane control block pipe/ connectors are to be renewed as in poor condition.","Deck Mach.","Structural Condn. / WT integrity ","Equipment Related","","","","","Inspection carried out, connectors cleaned , no leaky from connectors.","2019-07-30","","Completed","2019-07-17","No","No","No","Internal"]
[null,null,null,null,5104,"27/10/2019 6:55:29 AM","2019-05-15","Observation","Ship Staff","Ship Staff Insp.","SUPPORT PIPE FOR MOORING WINCH OPERATOR STANDING PLATFORM HOLED AND WASTED FOR STERN MOORING WINCH NO 7","Mooring Mach.","Mooring","Equipment Related","","","","","COLD WORK REPAIR CARRIED OUT. STRENGTHEN THE SUPPORT PIPE AND PAINTING.","2019-08-15","","Completed","2019-07-29","No","No","No","Internal"]
[null,null,null,null,5105,"27/10/2019 6:58:51 AM","2019-07-13","Deficiency","Ship Staff","Ship Staff Insp.","DECK SEAL FLANGE FOR HIGH LEVEL SENSOR HOUSING HOLED.","Inert Gas","Cargo / Ballast Systems","Equipment Related","","","","","NEW FLANGE FABRICATED.","2019-08-15","","Completed","2019-07-18","No","No","No","Internal"]
[null,null,null,null,5106,"27/10/2019 7:08:14 AM","2019-07-13","Deficiency","Ship Staff","Ship Staff Insp.","GANGWAY PORT SIDE LEVER BODY FOR SWING IN/OUT BROKEN.","Deck Mach.","Structural Condn. / WT integrity ","Equipment Related","","","","","SPARE LEVER BODY REPLACED AND TRIED OUT.","2019-08-15","","Completed","2019-07-25","No","No","No","Internal"]
[null,null,null,null,5107,"27/10/2019 7:11:55 AM","2019-07-13","Deficiency","Ship Staff","Ship Staff Insp.","CARGO MANIFOLD PORT AND STBD GAUGE COCKS WHEELS BROKEN.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","WHEELS FABRICATED AND INSTALLED.","2019-07-15","","Completed","2019-07-28","No","No","No","Internal"]
[null,null,null,null,5108,"27/10/2019 12:46:53 PM","2019-05-09","Observation","Ship Staff","Ship Staff Insp.","AC compressor sump oil needs to be replaced","Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Oil renewed","2019-08-08","","Completed","2019-07-22","No","No","No","Internal"]
[null,null,null,null,5109,"27/10/2019 12:52:41 PM","2019-07-03","Deficiency","Ship Staff","Ship Staff Insp.","PORT windlass FWD motor has excessive hydaulic oil leak.","Mooring Mach.","Mooring","Equipment Related","","","","","Forward motor complet overhauling carried out.","2019-08-15","","Completed","2019-07-22","No","No","No","Internal"]
[null,null,null,null,5110,"27/10/2019 12:54:07 PM","2019-07-19","Observation","Ship Staff","Ship Staff Insp.","No1 boiler starboard gauge glass leaky","Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","Gauge glass renewed","2019-08-30","","Completed","2019-07-20","No","No","No","Internal"]
[null,null,null,null,5111,"27/10/2019 12:56:53 PM","2019-04-25","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Winch 4,7 wire end securing hook bent.To be repaired.","Mooring Mach.","Mooring","Equipment Related","","","","","Repaired.","2019-07-25","","Completed","2019-07-25","No","No","No","Internal"]
[null,null,null,null,5112,"27/10/2019 12:58:28 PM","2019-04-25","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Valves for AC condensers, Steam condensers and Boiler water circulation P/P outlet to No.1 are not holding. Same to be repaired/renewed","Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Valves for AC condenser remaining","2019-07-30","","Completed","2019-07-31","No","No","No","Internal"]
[null,null,null,null,5113,"27/10/2019 1:01:45 PM","2018-12-11","Deficiency","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Side) located in China passage was found broken.","Hull & Tanks","Structural Condn. / WT integrity ","Equipment Related","","","","","Bracket renewed","2019-08-30","","Completed","2019-08-05","No","No","No","Internal"]
[null,null,null,null,5114,"27/10/2019 1:03:10 PM","2019-08-06","Observation","Ship Staff","Ship Staff Insp.","MSB room AC sea water inlet pipe holed","ER Pipes, valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","pipe section to be renewed","2019-08-15","","Completed","2019-08-07","No","No","No","Internal"]
[null,null,null,null,5115,"27/10/2019 1:04:41 PM","2019-08-06","Observation","Ship Staff","Ship Staff Insp.","ECR AC sea water inlet pipe holed","ER Pipes, valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Pipe section to be renewed","2019-08-15","","Completed","2019-08-07","No","No","No","Internal"]
[null,null,null,null,5116,"27/10/2019 1:09:30 PM","2019-08-06","Observation","Ship Staff","Ship Staff Insp.","Control air has too much water content","Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Control air drier filter to be cleaned","2019-08-15","","Completed","2019-08-06","No","No","No","Internal"]
[null,null,null,null,5117,"27/10/2019 1:12:27 PM","2019-08-06","Observation","Ship Staff","Ship Staff Insp.","Water leaking from hydroblaster shaft","Miscellaneous","General Appearance","Equipment Related","","","","","Oring to be renewed.","2019-08-15","","Completed","2019-08-06","No","No","No","Internal"]
[null,null,null,null,5118,"27/10/2019 1:17:41 PM","2019-04-25","Observation","Ship Staff","Suptd. Insp.","Mesh of pump room blower are in poor condition.Mesh to removed, the frame from inside to chipped and painted and new mesh is to installed.","Hull & Tanks","Structural Condn. / WT integrity ","Equipment Related","","","","","Pumproom blower complete derusting. Two coats primer and final coat carried out.","2019-08-30","","Completed","2019-08-10","No","No","No","Internal"]
[null,null,null,null,5119,"27/10/2019 1:24:59 PM","2019-04-25","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Hydraulic boxes forward to be blasted and painted red. The boxes are also to be derusted and painted from the bottam as it was seen on the boxes where blasting has been done the bottom...................... ","Miscellaneous","General Appearance","Equipment Related","","","","","All hydraulic boxes on deck completed derusting two coats primer and final coat.","2019-08-12","","Completed","2019-08-09","No","No","No","Internal"]
[null,null,null,null,5120,"27/10/2019 1:28:03 PM","2019-07-13","Observation","Ship Staff","Ship Staff Insp.","Garbage bins at garbage point not seal tight.","Miscellaneous","General Appearance","Equipment Related","","","","","Hing and securing arrangement prepared.","2019-08-15","","Completed","2019-08-10","No","No","No","Internal"]
[null,null,null,null,5121,"27/10/2019 1:32:57 PM","2019-08-06","Deficiency","Ship Staff","Ship Staff Insp.","Mooring winch MW5 inlet line holded.","Mooring Mach.","Mooring","Equipment Related","","","","","Inlet pipeline to dimantel and welded and fixed back in position.","2019-08-15","","Completed","2019-08-10","No","No","No","Internal"]
[null,null,null,null,5122,"27/10/2019 1:35:36 PM","2019-08-06","Observation","Ship Staff","Ship Staff Insp.","Mooring winch MW6 inlet line valve leaking.","Mooring Mach.","Mooring","Equipment Related","","","","","Inlet valve to repair and fixed back.","2019-08-15","","Completed","2019-08-10","No","No","No","Internal"]
[null,null,null,null,5123,"27/10/2019 1:39:36 PM","2019-06-27","Deficiency","Ship Staff","Ship Staff Insp.","STBD windlass pinion and gear slipping at particular instances.","Mooring Mach.","Mooring","Equipment Related","","","","","To check the backlash of gear checked and both pinion bearings renewed.","2019-07-30","","Completed","2019-08-12","No","No","No","Internal"]
[null,null,null,null,5124,"27/10/2019 1:44:00 PM","2019-07-05","Deficiency","Ship Staff","Ship Staff Insp.","STBD windlass aft motor end cover wasted.","Mooring Mach.","Mooring","Equipment Related","","","","","Reqn, Raised for new cover.Temparory repairs carried out and motor tried out found no leak.","2019-08-30","RESP190056","Completed","2019-08-12","No","No","No","Internal"]
[null,null,null,null,5125,"27/10/2019 1:45:55 PM","2019-02-28","Deficiency","Ship Staff","Ship Staff Insp.","AE JW cooler 2- SW inlet valve not holding. To be replaced with spare","ER Pipes, valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Awaiting for anchorage","2019-08-30","","Completed","2019-08-30","No","No","No","Internal"]
[null,null,null,null,5126,"27/10/2019 1:47:33 PM","2019-04-25","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ME fuel p/p's- all umbrella seals have been reported are leaking. To be investigated","Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Investigation carried out foud no seal leak","2019-07-30","","Completed","2019-08-21","No","No","No","Internal"]
[null,null,null,null,5127,"27/10/2019 1:49:08 PM","2019-04-25","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","It has been reported by CE that CLO consumption from Alpha lubricator stroke calculations is not matching with actual","Main Engine ","Eng. / Strg. Comp.","Equipment Related","","","","","Investigation carried out. Found calculation is matching","2019-08-24","","Completed","2019-08-21","No","No","No","Internal"]
[null,null,null,null,5128,"27/10/2019 1:51:02 PM","2019-04-25","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Coverings on ECR chairs are torn. Same to be renewed","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","No rexin available on board, item will be added to ER store requisition","2019-07-30","RESP190063","Completed","2019-08-25","No","No","No","Internal"]
[null,null,null,null,5129,"27/10/2019 1:56:21 PM","2019-08-30","Observation","Ship Staff","Ship Staff Insp.","AE LT cooler sea water pipe section damaged","Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Pipe section renewed","2019-08-30","","Completed","2019-08-30","No","No","No","Internal"]
[null,null,null,null,5130,"27/10/2019 1:58:06 PM","2019-04-25","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","IG automation is not working. Transmitter is on order. To be rectified as soon as spares are received.","Inert Gas","Eng. / Strg. Comp.","Equipment Related","","","","","Transmitter renewed","2019-07-15","","Completed","2019-08-25","No","No","No","Internal"]
[null,null,null,null,5131,"27/10/2019 2:01:50 PM","2019-04-25","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Hydraulic pipes connecting the hydraulic motors on mooring winches are in very poor condition. New pipes to be fabricated and renewed.","Mooring Mach.","Mooring","Equipment Related","","","","","some pipe renewed.","2019-08-30","","Completed","2019-08-20","No","No","No","Internal"]
[null,null,null,null,5132,"27/10/2019 2:05:41 PM","2019-04-25","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Gas tight UTI- only ONE more to be supplied.","Miscellaneous","Cargo / Ballast Systems","Equipment Related","","","","","Awaiting Supply. To be procured directly from office.","2019-08-15","","Completed","2019-08-24","No","No","No","Internal"]
[null,null,null,null,5133,"27/10/2019 3:20:25 PM","2019-04-25","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Vessel does not have spare wire for: Hose handling crane, gangway and lifeboat.Same to be.","Deck Mach.","Mooring","Equipment Related","","","","","Recevied in Singapore.","2019-08-15","RESP195062","Completed","2019-08-23","No","No","No","Internal"]
[null,null,null,null,5134,"27/10/2019 3:24:28 PM","2019-05-08","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","WS lathe machine should fabricate transparent safety shield to avoid injury to eye of personnel carrying out the job.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","No transparent safety shield available on board, item will be added to ER store requisition.","2019-06-05","RESP190064","Completed","2019-08-29","No","No","No","Internal"]
[null,null,null,null,5135,"27/10/2019 3:27:04 PM","2019-08-23","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","MW7 in poop deck is leaking from flange.","Mooring Mach.","Mooring","Equipment Related","","","","","Hydraulic leak rectified.","2019-09-22","","Completed","2019-09-03","No","No","No","Internal"]
[null,null,null,null,5136,"27/10/2019 3:30:31 PM","2019-08-27","Deficiency","Ship Staff","Ship Staff Insp.","Observed two holes in STBD side pilot ladder pneumatic line.","Deck Mach.","Structural Condn. / WT integrity ","Equipment Related","","","","","Section disconnected, repaired and fitted back.","2019-09-10","","Completed","2019-09-05","No","No","No","Internal"]
[null,null,null,null,5137,"27/10/2019 3:32:39 PM","2019-08-23","Observation","Ship Staff","Ship Staff Insp.","Unit 7 and 5 were found dry during the scavenge inspection. The CLO lubrication to be increased for these units and closely monitored","Main Engine ","Eng. / Strg. Comp.","Equipment Related","","","","","CLO setting increased","2019-08-30","","Completed","2019-08-26","No","No","No","Internal"]
[null,null,null,null,5138,"27/10/2019 3:38:02 PM","2019-09-11","Observation","Ship Staff","Ship Staff Insp.","Starboard side pilot ladder air motor operating lever not working.","Deck Mach.","Emgcy. Systems","Equipment Related","","","","","Same overhauled and working satisfactory.","2019-09-20","","Completed","2019-09-12","No","No","No","Internal"]
[null,null,null,null,5139,"27/10/2019 3:39:48 PM","2019-08-23","Observation","Ship Staff","Ship Staff Insp.","Arrangement for waer washing of AE turbocharger does not have a drain arrangement","Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","As per manual no drain but water flow regulating valve to maintain the flow. Cycle carried out 3 times based on........","2019-10-22","","Completed","2019-08-23","No","No","No","Internal"]
[null,null,null,null,5140,"27/10/2019 3:42:02 PM","2019-09-11","Observation","Ship Staff","Ship Staff Insp.","AE3 LT pump oil seal leaky","Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Pump overhauled","2019-09-20","","Completed","2019-09-12","No","No","No","Internal"]
[null,null,null,null,5141,"27/10/2019 3:44:33 PM","2019-08-23","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Noon log alarm printer in ECR not working","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","noon log printer working satisfactorily","2019-10-22","","Completed","2019-09-13","No","No","No","Internal"]
[null,null,null,null,5142,"27/10/2019 3:46:20 PM","2019-08-26","Observation","Ship Staff","Ship Staff Insp.","ECR noon log printer not working","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","cartridge renewed","2019-11-20","","Completed","2019-09-12","No","No","No","Internal"]
[null,null,null,null,5143,"27/10/2019 3:50:19 PM","2019-08-23","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Covers for the hydraulic boxes on deck have not been blasted and painted from the bottom at the.........","Deck Mach.","General Appearance","Equipment Related","","","","","Same to carried out.Silica get to be placed inside the boxes.","2019-11-22","","Completed","2019-09-20","No","No","No","Internal"]
[null,null,null,null,5144,"27/10/2019 4:14:53 PM","2019-08-26","Observation","Ship Staff","Ship Staff Insp.","No.1 ballast pump mechanical seal leak. ","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","Seal renewed.","2019-09-30","","Completed","2019-09-23","No","No","No","Internal"]
[null,null,null,null,5145,"27/10/2019 4:16:52 PM","2019-09-25","Observation","Ship Staff","Ship Staff Insp.","Main engine T/C grid wash line got choked","Main Engine ","Eng. / Strg. Comp.","Equipment Related","","","","","Same cleared","2019-09-30","","Completed","2019-09-29","No","No","No","Internal"]
[null,null,null,null,5146,"27/10/2019 4:18:09 PM","2019-09-25","Observation","Ship Staff","Ship Staff Insp.","AE jacket water temp are not maintaining with one jacket cooler in use.","Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Both AE jacket cooler plates are cleaned","2019-11-20","","Completed","2019-09-25","No","No","No","Internal"]
[null,null,null,null,5147,"27/10/2019 4:20:28 PM","2019-09-20","Observation","Ship Staff","Ship Staff Insp.","Hydro blaster not building up pressure.","Miscellaneous","General Appearance","Equipment Related","","","","","All seal are renewed.","2019-09-22","","Completed","2019-09-22","No","No","No","Internal"]
[null,null,null,null,5148,"27/10/2019 4:21:59 PM","2019-04-01","Deficiency","Ship Staff","Ship Staff Insp.","Boiler feed pumps no2 heavy vibrations and seal leak","Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","pump overhauled","2019-08-30","RESP190035","Completed","2019-09-28","No","No","No","Internal"]
[null,null,null,null,5149,"27/10/2019 4:25:03 PM","2019-04-01","Deficiency","Ship Staff","Ship Staff Insp.","Port gangway shifting motor not working.","Deck Mach.","Emgcy. Systems","Equipment Related","","","","","Fitted and working satisfactory.","2019-09-10","RESP195075","Completed","2019-09-20","No","No","No","Internal"]
[null,null,null,null,5150,"27/10/2019 4:26:26 PM","2019-04-05","Deficiency","Ship Staff","Ship Staff Insp.","Valve no: 265(V11) - Super Spool Pneumatic Direction valve (Type: PSMT - 33) for puncture valve actuator for each unit found leaking.","Main Engine ","Eng. / Strg. Comp.","Equipment Related","","","","","Leak rectified","2019-10-15","","Completed","2019-10-19","No","No","No","Internal"]
[null,null,null,null,5151,"27/10/2019 4:27:47 PM","2019-04-05","Deficiency","Ship Staff","Ship Staff Insp.","Reducing valve no: 59 and valve no 45 found leaking on Main Engine Pneumatic control system","Main Engine ","Eng. / Strg. Comp.","Equipment Related","","","","","Leaky valve renewed","2019-10-15","","Completed","2019-10-14","No","No","No","Internal"]
[null,null,null,null,5152,"27/10/2019 4:30:44 PM","2019-04-25","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Manoeuvring system VIT valves require overhauling. Kits are on order same to be renewed","Main Engine ","Eng. / Strg. Comp.","Equipment Related","","","","","Leaky valves renewed","2019-10-15","","Completed","2019-10-14","No","No","No","Internal"]
[null,null,null,null,5153,"27/10/2019 4:36:18 PM","2019-08-23","Observation","Ship Staff","Ship Staff Insp.","Auxboiler no2 steam stop valve gland is leaking. To be rectified.","Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","Bonnet gasket renewed. Leak rectified.","2019-10-22","","Completed","2019-10-16","No","No","No","Internal"]
[null,null,null,null,5154,"27/10/2019 4:37:35 PM","2019-10-13","Observation","Ship Staff","Ship Staff Insp.","Boiler no1 FO tracing steam valve leaky","Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","Valve renewed","2019-10-15","","Completed","2019-10-16","No","No","No","Internal"]
[null,null,null,null,5155,"27/10/2019 4:38:59 PM","2019-10-12","Observation","Ship Staff","Ship Staff Insp.","Main engine cylinder head jack leaky","Main Engine ","Eng. / Strg. Comp.","Equipment Related","","","","","O ring and back up ring renewed","2019-10-12","","Completed","2019-10-12","No","No","No","Internal"]
[null,null,null,null,5156,"27/10/2019 4:42:10 PM","2019-10-05","Observation","Ship Staff","Ship Staff Insp.","Control air pressure reducing valve leaky","Air Comp.","Eng. / Strg. Comp.","Equipment Related","","","","","Same overhauled","2019-10-05","","Completed","2019-10-05","No","No","No","Internal"]
[null,null,null,null,5157,"27/10/2019 4:45:25 PM","2019-04-25","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Ladder step on the mainfold are in poor condition.These are to be repaired.","Deck Pipe / Fittings","General Appearance","Equipment Related","","","","","Both PORT & STBD manifolds de- rusted and painted including ladders.","2019-10-30","","Completed","2019-10-13","No","No","No","Internal"]
[null,null,null,null,5158,"27/10/2019 4:40:24 PM","2019-10-10","Observation","Ship Staff","Ship Staff Insp.","FWG distillate pump discharge line got holed","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","Same renewed","2019-10-10","","Completed","2019-10-10","No","No","No","Internal"]
[null,null,null,null,5842,"2019-11-03 19:51:10.000","2019-10-14","Observation","Ship Staff","Ship Staff Insp.","Boiler Forward gauge glass leaky","Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Leak rectified","2019-10-20","","Completed","2019-10-16","No","No","No","Internal"]
[null,null,null,null,5843,"2019-11-03 19:58:03.000","2019-10-05","Observation","Ship Staff","Ship Staff Insp.","ME unit #2, #4aft high pressure pipe leaky","Main Engine ","Eng. / Strg. Comp.","Equipment Related","10.12","Very High","","","Same overhauled and leak rectified","2019-10-10","","Completed","2019-10-07","No","No","No","Internal"]
[null,null,null,null,5844,"2019-11-03 20:06:10.000","2019-10-18","Observation","Ship Staff","Ship Staff Insp.","AE Jacket cooler SW pipe section found leaky","ER Pipes, valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.31","Very High","","","Same rectified","2019-10-20","","Completed","2019-10-19","No","No","No","Internal"]
[null,null,null,null,null,"24/10/2019 7:15:36 PM","2019-05-21","Observation","Ship Staff","Ship Staff Insp.","Unit no. 7 top piston ring broken at butt.","Main Engine ","Eng. / Strg. Comp.","Equipment Related",10.119999999999999,"Very High","Not Applicable","Not Applicable","Piston renewed with overhauled, ring renewed.","2019-11-15",null,"Completed","2019-11-11","No",null,null,"Internal"]
[null,null,null,null,null,43766.273877314816,"2019-08-27","Observation","Ship Staff","Ship Staff Insp.","Unit no 2 top piston ring broken at butt","Main Engine ","Eng. / Strg. Comp.","Equipment Related",null,null,"Not Applicable","Not Applicable","piston renewed with overhauled spare piston and piston rings are renewed","2019-11-30",null,"Completed","2019-11-07","No",null,null,"Internal"]
[null,null,null,null,null,43766.278055555558,"2019-09-11","Observation","Ship Staff","Ship Staff Insp.","Unit no5 top piston ring broken at butt","Main Engine ","Eng. / Strg. Comp.","Equipment Related",null,null,"Not Applicable","Not Applicable","Piston rings were renewed.","2019-11-20",null,"Completed","2019-11-05","No",null,null,"Internal"]
[null,null,null,null,null,"20/12/2019 7:45:39 AM","2019-11-16","Observation","Ship Staff","Ship Staff Insp.","Atm condenser sea water outlet pipe leak.","ER Pipes, valves & fittings","Eng. / Strg. Comp.","Equipment Related",8.11,"Medium","Not Applicable","Not Applicable","Pipe leak rectified and inlet and outlet valve which was not holding renewed with new spare.","2019-11-20",null,"Completed","2019-11-16","No",null,null,"Internal"]
[null,null,null,null,null,"20/12/2019 7:50:34 AM","2019-11-17","Breakdown","Ship Staff","Ship Staff Insp.","Sea water service pump no 2 mechanical seal leak","Aux. Mach.,Miscellaneous","Eng. / Strg. Comp.","Equipment Related",8.11,"Medium","Not Applicable","Not Applicable","pump overhauled","2019-11-18",null,"Completed","2019-11-18","No",null,null,"Internal"]
[null,null,null,null,null,"20/12/2019 7:54:05 AM","2019-11-20","Observation","Ship Staff","Ship Staff Insp.","Main cooling sea water pump no 2 mechanical seal leak","Aux. Mach.","Eng. / Strg. Comp.","Equipment Related",8.11,"Medium","Not Applicable","Not Applicable","pump overhauled","2019-11-21",null,"Completed","2019-11-21","No",null,null,"Internal"]
[null,null,null,null,null,"20/12/2019 8:10:49 AM","2019-04-16","Observation","SIRE / CDI Insp.","OM Insp. (Eg. SIRE, CDI etc.)","No evidence showing regulators located at Oxygen & Acetylene cylinders side were inspected annually and replaced/refurbished 5Y basis as per manufacturers instructions","Miscellaneous","General Appearance","Equipment Related",5.26,"Medium","Not Applicable","Not Applicable","Regulators inspected and a record generated serving as a proof of the same being done.","2019-05-31",null,"Completed","2019-05-10","No",null,null,"External"]
[null,null,null,null,null,"20/12/2019 8:16:07 AM","2019-05-07","Deficiency","PSC Insp.","PSC Inspection","Three E/R dampers when in closed position found gaps of atleast 3mm at intervals, thus unable to provide effective isolation during emergency","Miscellaneous","Emgcy. Systems","Equipment Related",5.35,"Medium","Fire safety","Asia and the Pacific","Dampers repaired, operation tested and sighted by Class inspector. Found in good working condition.","2019-05-07",null,"Completed","2019-05-07","No",null,null,"External"]
[null,null,null,null,null,"20/12/2019 8:19:43 AM","2019-05-07","Deficiency","PSC Insp.","PSC Inspection","Emergency generator DO tank air vent found severely corroded and hole.","Critical Equip.","Emgcy. Systems","Equipment Related",11.7,"High","Fire safety","Asia and the Pacific","Air vent repaired and verified by Class inspector.","2019-05-07",null,"Completed","2019-05-07","No",null,null,"External"]
[null,null,null,null,null,"20/12/2019 8:23:52 AM","2019-08-20","Deficiency","SIRE / CDI Insp.","OM Insp. (Eg. SIRE, CDI etc.)","1 SCBA bottle unit for Helicopter equipment stowed inside midship locker store was noted with defective demand valve whilst testing.","LSA / FFA","LSA / FFA Appliances","Equipment Related",5.43,"High","Not Applicable","Not Applicable","New demand valve received in Singapore and fitted.","2019-08-31",null,"Completed","2019-08-23","No",null,null,"External"]
[null,null,null,null,null,"20/12/2019 8:28:55 AM","2019-02-12","Observation","Ship Staff","Nav Audit / Verification","Astronomical sights not being practised regularly.","Nav & comm. equip.","Navigation","Human Error",4.2,"Medium","Not Applicable","Not Applicable","All deck officers were instructed to follow company procedures and practice astronomical sights as when weather favours. Sights were practised by all officers and are familiar with use of sextant and calculations.","2019-03-31",null,"Completed","2019-03-27","No",null,null,"Internal"]
[null,null,null,null,null,"20/12/2019 8:35:48 AM","2019-08-21","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Entries in the cargo log not in line with the recommended entries mention at the start of the book. No record of cross-checks made by OOW for the line ups.","Cargo Mach.","Cert. & Docu.","Human Error",8.5,"Very High","Not Applicable","Not Applicable","Standard guidelines provided by company regarding entry in log books has been discussed and followed. During Pre-Arrival cargo meeting same to be discussed always.","2019-09-30",null,"Completed","2019-09-13","No",null,null,"Internal"]
[null,null,null,null,null,"20/12/2019 11:09:43 AM","2019-08-21","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","MBL markings not present on the mooring winches (Refer Mooring equipment guidelines 4)","Mooring Mach.","Mooring","Knowledge Based",9.6999999999999993,"Medium","Not Applicable","Not Applicable","MEG Ed.4 has been referred and the required markings carried out. ","2019-09-30",null,"Completed","2019-09-14","No",null,null,"Internal"]
[null,null,null,null,null,"20/12/2019 11:48:09 AM","2019-08-28","Observation","Owner / Marine / Tech. Suptd.","Nav Audit / Verification","Only the internal history of the FE800 Furuno Echosounder is available, No external recording facility available  ","Nav & comm. equip.","Navigation","Equipment Related",4.1900000000000004,"Low","Not Applicable","Not Applicable","The vessel has a Data recroding software (FE800 DATA RECORDING SYSTEM) which is malfunctioning after the upgradation of the Personal computer to Windows 7 OS. Vessel is working on resolving the isue so as to enable data saving facility for future referance. Vessel has raised a servie requisition for IT support to rectify the issue. \r\nHowever, for the time being the echo sounder data is being recorded by the Master ECDIS which can save the data for 90 days and the vessel is writing down the depths at critical stages in the Bridge bell book. ","2019-09-15",null,"Completed","2019-09-12","No",null,null,"Internal"]
[null,null,null,null,null,"20/12/2019 11:50:31 AM","2019-08-28","Observation","Owner / Marine / Tech. Suptd.","Nav Audit / Verification","Pre Departure tests and checks for GMDSS equipment not carried out. \r\nDeparture steering gear tests: 3 monthly steering gear (due on 23rd Aug 2019) not carried out","Nav & comm. equip.","Navigation","Human Error",4.2300000000000004,"High","Not Applicable","Not Applicable","-Steering gear test carried out on first available oppurtunity as per regulations. \r\nFound in good working order. \r\nNecessary entries made and the test was documented. \r\n-GMDSS departure tests carried out as well by the GMDSS officer. GMDSS Officer instructed to not let such a lapse occur again and to ensure that the pre departure tests are carried out diligently. ","2019-09-15",null,"Completed","2019-09-12","No",null,null,"Internal"]
[null,null,null,null,null,"20/12/2019 11:54:08 AM","2019-08-28","Observation","Owner / Marine / Tech. Suptd.","Nav Audit / Verification","Celestial observations were not practiced by each member of the bridge team ","Nav & comm. equip.","Navigation","Human Error",4.2,"Medium","Not Applicable","Not Applicable","Celestial observations practised by all OOW and logged down. \r\nComparison has been carried out with the position obtained by the Celestial observation and the GPS position at that instant. Error deemed to be slight and acceptable. ","2019-09-15",null,"Completed","2019-09-12","No",null,null,"Internal"]
[null,null,null,null,null,"20/12/2019 11:56:25 AM","2019-08-29","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","LSA Training manual data not ship specific : Location / Quantity of equipment , Procedure to use the recovery strops/ recover Rescue boat in rough weather missing","LSA / FFA","Cert. & Docu.","Inappropriate Procedure",5.34,"Low","Not Applicable","Not Applicable","-All the LSA/FFA equipments location and quantities inserted against the relevant equipments pages.\r\n-Procedure for recovery of rescue boat in rough weather inserted in the Training Manuals.","2019-09-30",null,"Completed","2019-09-13","No",null,null,"Internal"]
[null,null,null,null,null,"20/12/2019 11:58:37 AM","2019-08-29","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Life jacket markings not in line with SOLAS (\"Front\" missing on all life jackets excluding the oversize and child located in the Fire station. A few of them do not have the standard/ resolution to which they confirm)","LSA / FFA","LSA / FFA Appliances","Equipment Related",5.33,"High","Not Applicable","Not Applicable","-Officer incharge immediately marked all lifejackets with FRONT markings.\r\n-Rest all the markings were cross verified with SOLAS standards.","2019-09-30",null,"Completed","2019-08-30","No",null,null,"Internal"]
[null,null,null,null,null,"20/12/2019 12:03:38 PM","2019-08-29","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Helicopter Landing Area markings not in compliance with the IACS guide ","Hull & Tanks","General Appearance","Inappropriate Procedure",11.3,"Medium","Not Applicable","Not Applicable","PROPER GUIDELINES HAVE BEEN REFERRED IN IACS GUIDE FOR MARKING IN HELICOPTER LANDING AREA AND CARRIED OUT.","2019-09-30",null,"Completed","2019-09-13","No",null,null,"Internal"]
[null,null,null,null,null,"20/12/2019 12:10:36 PM","2019-08-29","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","VL Load\" marking of the P/S hose saddles and Port side manifold Drp tray capaicty marking missing. ","Miscellaneous","General Appearance","Inappropriate Procedure",9.19,"Low","Not Applicable","Not Applicable","THE VL LOAD  AND THE MANIFOLD DRIP TRAY CAPACITY HAS BEEN MARKED.","2019-09-30",null,"Completed","2019-09-30","No",null,null,"Internal"]
[null,null,null,null,null,"20/12/2019 12:12:39 PM","2019-10-02","Observation","Ship Staff","Nav Audit / Verification","Procedure for downloading VDR data forgotten/not conversant with some members of the Bridge team as a few members of the Bridge team are relatively new. ","Nav & comm. equip.","Navigation","Human Error",4.1100000000000003,"Medium","Not Applicable","Not Applicable","A VDR Drill has been reconducted and the entire Bridge team has been quizzed post the drill on the procedure to retrieve the data so as to ensure thorough understanding of the same. ","2019-10-30",null,"Completed","2019-10-19","No",null,null,"Internal"]

{"sheet":"Calc","index":2,"n_rows":28,"n_cols":12,"rows_kept":28,"cut":false,"hidden":true,"merged":[]}
["Def_type","Def_cause","Equipments","VIQrefno","Observer_code"]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,"Dim itemSele As Long"]
[null,null,null,null,null,null,null,null,null,null,null,"   dim startRow as integer"]
[null,null,null,null,null,null,null,null,null,null,null,"   startRow=1"]
[null,null,null,null,null,null,null,null,null,null,null,"        For itemSele = 0 To ListBox1.ListCount - 1"]
[null,null,null,null,null,null,null,null,null,null,null,"        If ListBox1.Selected(itemSele) = True Then"]
[null,null,null,null,null,null,null,null,null,null,null,"        Worksheets(\"WorksheetName\").Range(\"A\" & startRow).Value = ListBox1.List(itemSele)"]
[null,null,null,null,null,null,null,null,null,null,null,"        startRow = startRow + 1"]
[null,null,null,null,null,null,null,null,null,null,null,"        End If"]
[null,null,null,null,null,null,null,null,null,null,null,"        Next"]
[null,null,null,null,null,null,null,null,null,null,null,"Dim LastRowA As String"]
[null,null,null,null,null,null,null,null,null,null,null,"        Dim itemSele As Long"]
[null,null,null,null,null,null,null,null,null,null,null,"       Dim startRow as integer"]
[null,null,null,null,null,null,null,null,null,null,null,"        LastRowA = ActiveSheet.Cells(Rows.count, \"A\").End(xlUp).row"]
[null,null,null,null,null,null,null,null,null,null,null,"        startQue = 0"]
[null,null,null,null,null,null,null,null,null,null,null,"        For itemSele = 0 To ListBox1.ListCount - 1"]
[null,null,null,null,null,null,null,null,null,null,null,"        For startRow = 1 To LastRowA"]
[null,null,null,null,null,null,null,null,null,null,null,"        If Worksheets(\"WorksheetName\").Range(\"A\" & startRow).Value = ListBox1.List(itemSele) Then"]
[null,null,null,null,null,null,null,null,null,null,null,"        ListBox1.Selected(itemSele) = True"]
[null,null,null,null,null,null,null,null,null,null,null,"        Exit For"]
[null,null,null,null,null,null,null,null,null,null,null,"        End If"]
[null,null,null,null,null,null,null,null,null,null,null,"        Next j"]
[null,null,null,null,null,null,null,null,null,null,null,"        Next"]
[null,null,null,null,null,null,null,null,null,null,null,"        End If"]

{"sheet":"Areaofobs","index":3,"n_rows":17,"n_cols":2,"rows_kept":17,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Cargo / Ballast Systems",11]
["Cert. & Docu.",2]
["Communication",6]
["Crew Management",3]
["Emgcy. Systems",13]
["Eng. / Strg. Comp.",14]
["General Appearance",15]
["Ice Opns.",17]
["LSA / FFA Appliances",8]
["MLC Related",4]
["Mooring",12]
["Navigation",5]
["MARPOL Related",9]
["ISM Related",7]
["ISPS Related",10]
["Structural Condn. / WT integrity ",16]

{"sheet":"Vessel_type","index":4,"n_rows":1,"n_cols":2,"rows_kept":1,"cut":false,"hidden":true,"merged":[]}
["Vessel_type","ID"]

{"sheet":"Deficiency_type","index":5,"n_rows":9,"n_cols":3,"rows_kept":9,"cut":false,"hidden":true,"merged":[]}
["TITLE","Type of deficiency_description","ID"]
["Breakdown",null,6]
["Condn of Class / Memo",null,5]
["Critical Equipment",null,4]
["Deficiency",null,1]
["Guarantee Claim",null,8]
["Non Conformity",null,2]
["Observation",null,3]
["Other",null,7]

{"sheet":"VIQrefno","index":6,"n_rows":427,"n_cols":3,"rows_kept":427,"cut":false,"hidden":true,"merged":[]}
["VIQ_ref_no","Risk Value of observation","ID"]
["1.1","Low",8243]
["1.10","Low",8252]
["1.11","Low",8253]
["1.12","Low",8254]
["1.13","Low",8255]
["1.14","Low",8256]
["1.15","Low",8257]
["1.16","Low",8259]
["1.17","Low",8260]
["1.18","Low",8261]
["1.19","Low",8262]
["1.2","Low",8244]
["1.20","Low",8263]
["1.21","Low",8265]
["1.22","Low",8266]
["1.23","Low",8267]
["1.24","Low",8268]
["1.25","Low",8269]
["1.26","Low",8270]
["1.3","Low",8245]
["1.4","Low",8246]
["1.5","Low",8247]
["1.6","Low",8248]
["1.7","Low",8249]
["1.8","Low",8250]
["1.9","Low",8251]
["1.99","High",11258]
["10.1","Medium",8461]
["10.10","High",8470]
["10.11","Medium",8471]
["10.12","Very High",8472]
["10.13","Very High",8473]
["10.14","Medium",8474]
["10.15","Low",8475]
["10.16","Very High",8476]
["10.17","Very High",8477]
["10.18","High",8478]
["10.19","Very High",8479]
["10.2","Low",8462]
["10.20","High",8480]
["10.21","Medium",8481]
["10.22","Low",8482]
["10.23","Medium",8483]
["10.24","Low",8484]
["10.25","Very High",8485]
["10.26","High",8486]
["10.27","Medium",8487]
["10.28","Low",8488]
["10.29","Medium",8489]
["10.3","Medium",8463]
["10.30","High",8490]
["10.31","Very High",8491]
["10.32","Very High",8492]
["10.33","High",8493]
["10.34","High",8494]
["10.35","Very High",8495]
["10.36","Very High",8496]
["10.37","Medium",8497]
["10.38","Medium",8498]
["10.39","High",8499]
["10.4","High",8464]
["10.40","Medium",8500]
["10.41","Medium",8501]
["10.42","Medium",8502]
["10.43","Medium",8503]
["10.44","Medium",8504]
["10.45","Very High",8505]
["10.46","High",8506]
["10.47","Medium",8507]
["10.48","High",8508]
["10.49","Medium",8509]
["10.5","Low",8465]
["10.50","High",8510]
["10.51","Low",8511]
["10.52","Medium",8512]
["10.53","Medium",8513]
["10.54","High",8514]
["10.55","Low",8515]
["10.6","Very High",8466]
["10.7","Medium",8467]
["10.8","Medium",8468]
["10.9","Medium",8469]
["10.99","High",8516]
["11.1","High",8420]
["11.10","Medium",8429]
["11.11","Very High",8430]
["11.12","Low",8431]
["11.13","Low",8432]
["11.14","Medium",8433]
["11.15","Low",8434]
["11.16","Low",8435]
["11.17","Low",8436]
["11.2","Medium",8421]
["11.3","Medium",8422]
["11.4","Very High",8423]
["11.5","Medium",8424]
["11.6","Medium",8425]
["11.7","High",8426]
["11.8","Low",8427]
["11.9","Low",8428]
["11.99","High",8437]
["12.1","High",8438]
["12.10","High",8448]
["12.11","High",8449]
["12.12","High",8450]
["12.13","High",8451]
["12.14","High",8452]
["12.15","High",8453]
["12.16","High",8454]
["12.17","High",8455]
["12.18","High",8456]
["12.19","High",8457]
["12.2","High",8439]
["12.20","High",8458]
["12.21","High",8459]
["12.3","High",8441]
["12.4","High",8442]
["12.5","High",8443]
["12.6","High",8444]
["12.7","High",8445]
["12.8","High",8446]
["12.9","High",8447]
["12.99","High",8460]
["2.1","Very High",8296]
["2.1.9","Very High",11259]
["2.10","Medium",8304]
["2.11","Medium",8305]
["2.12","Low",8306]
["2.13","Low",8307]
["2.14","Low",8308]
["2.15","Low",8309]
["2.16","Medium",8310]
["2.2","Medium",8297]
["2.3","High",8295]
["2.4","Medium",8298]
["2.5","Medium",8299]
["2.6","Low",8300]
["2.7","High",8301]
["2.8","High",8302]
["2.9","Medium",8303]
["2.99","High",8311]
["3.1","High",8312]
["3.2","Very High",8313]
["3.3","High",8314]
["3.4","Low",8294]
["3.5","Medium",8315]
["3.6","High",8316]
["3.7","Very High",8317]
["3.8","Very High",8318]
["3.99","High",8319]
["4.1","High",8320]
["4.10","High",8329]
["4.11","Medium",8330]
["4.12","Very High",8331]
["4.13","Very High",8332]
["4.14","Very High",8333]
["4.15","Very High",8334]
["4.16","Very High",8335]
["4.17","Very High",8336]
["4.18","Very High",8337]
["4.19","Low",8338]
["4.2","Medium",8321]
["4.20","Very High",8339]
["4.21","High",8340]
["4.22","Low",8341]
["4.23","High",8342]
["4.24","High",8343]
["4.25","Low",8344]
["4.26","Low",8345]
["4.27","High",8346]
["4.3","Medium",8322]
["4.4","High",8323]
["4.5","Very High",8324]
["4.6","Medium",8325]
["4.7","High",8326]
["4.8","Medium",8327]
["4.9","Medium",8328]
["4.99","High",8347]
["5.1","Very High",8517]
["5.10","High",8526]
["5.11","Low",8527]
["5.12","Medium",8528]
["5.13","High",8529]
["5.14","Very High",8530]
["5.15","Medium",8531]
["5.16","Very High",8532]
["5.17","Very High",8533]
["5.18","High",8534]
["5.19","Medium",8535]
["5.2","Very High",8518]
["5.20","Medium",8536]
["5.21","Medium",8537]
["5.22","High",8539]
["5.23","Very High",8540]
["5.24","Very High",8541]
["5.25","Medium",8542]
["5.26","Medium",8543]
["5.27","Medium",8544]
["5.28","Very High",8545]
["5.29","High",8546]
["5.3","Low",8519]
["5.30","High",8547]
["5.31","High",8548]
["5.32","High",8549]
["5.33","High",8550]
["5.34","Low",8551]
["5.35","Medium",8552]
["5.36","Low",8553]
["5.37","Low",8554]
["5.38","High",8555]
["5.39","Very High",8556]
["5.4","High",8520]
["5.40","Very High",8557]
["5.41","Very High",8558]
["5.42","Medium",8559]
["5.43","High",8560]
["5.44","High",8561]
["5.45","Medium",8564]
["5.46","Medium",8565]
["5.47","Medium",8566]
["5.48","Medium",8567]
["5.5","Low",8521]
["5.6","Low",8522]
["5.7","Medium",8523]
["5.8","Medium",8524]
["5.9","Very High",8525]
["5.99","High",8568]
["6.1","Medium",8348]
["6.10","Low",8357]
["6.11","High",8358]
["6.12","Medium",8359]
["6.13","Low",8360]
["6.14","High",8361]
["6.15","High",8362]
["6.16","Very High",8363]
["6.17","Very High",8364]
["6.18","Medium",8365]
["6.19","Low",8366]
["6.2","High",8349]
["6.20","Medium",8367]
["6.21","High",8368]
["6.22","Medium",8369]
["6.3","Low",8350]
["6.4","High",8351]
["6.5","Medium",8352]
["6.6","Medium",8353]
["6.7","High",8354]
["6.8","High",8355]
["6.9","Low",8356]
["6.99","High",8370]
["7.1","High",8371]
["7.10","High",8380]
["7.11","High",8381]
["7.12","High",8382]
["7.13","Medium",8383]
["7.14","Medium",8384]
["7.15","High",8385]
["7.16","High",8386]
["7.17","High",8387]
["7.2","High",8372]
["7.3","Low",8373]
["7.4","Low",8374]
["7.5","Low",8375]
["7.6","Medium",8376]
["7.7","Low",8377]
["7.8","High",8378]
["7.9","High",8379]
["7.99","High",8388]
["8.1","Very High",8569]
["8.10","Very High",8578]
["8.100","Low",11227]
["8.101","Medium",11228]
["8.102","Low",11229]
["8.103","Low",11230]
["8.104","Low",11231]
["8.105","Medium",11232]
["8.106","Medium",11233]
["8.107","Low",11234]
["8.108","High",11235]
["8.109","Very High",11236]
["8.11","Medium",8579]
["8.110","High",11237]
["8.111","Medium",11238]
["8.112","High",11239]
["8.113","Medium",11240]
["8.114","Low",11241]
["8.115","High",11242]
["8.116","Medium",11243]
["8.117","Medium",11244]
["8.118","Medium",11245]
["8.119","High",11246]
["8.12","Medium",8580]
["8.120","High",11247]
["8.121","Medium",11248]
["8.122","High",11249]
["8.123","High",11250]
["8.124","Low",11251]
["8.125","High",11252]
["8.126","Medium",11253]
["8.127","Medium",11254]
["8.13","Medium",8581]
["8.14","Very High",8582]
["8.15","High",8583]
["8.16","Very High",8584]
["8.17","Low",8585]
["8.18","High",8586]
["8.19","High",8587]
["8.199","High",11255]
["8.2","Medium",8570]
["8.20","Medium",8588]
["8.21","High",8589]
["8.22","Very High",8590]
["8.23","Medium",8591]
["8.24","Medium",8592]
["8.25","Very High",8593]
["8.26","High",8594]
["8.27","Medium",8595]
["8.28","Medium",8596]
["8.29","High",8598]
["8.3","Very High",8571]
["8.30","High",8599]
["8.31","High",8600]
["8.32","Low",8601]
["8.33","Medium",8602]
["8.34","High",8603]
["8.35","Medium",8604]
["8.36","Medium",8605]
["8.37","High",8607]
["8.38","Medium",8608]
["8.39","Medium",8609]
["8.4","Medium",8572]
["8.40","High",8610]
["8.41","Medium",8611]
["8.42","Medium",8612]
["8.43","Very High",8613]
["8.44","High",8615]
["8.45","High",8616]
["8.46","Very High",8617]
["8.47","Very High",8618]
["8.48","Medium",8619]
["8.49","High",8620]
["8.5","Very High",8573]
["8.50","Medium",8621]
["8.51","Low",8622]
["8.52","Low",8623]
["8.53","Low",8624]
["8.54","High",8625]
["8.55","Low",11182]
["8.56","Medium",11183]
["8.57","Medium",11184]
["8.58","High",11185]
["8.59","High",11186]
["8.6","Medium",8574]
["8.60","High",11187]
["8.61","Medium",11188]
["8.62","Very High",11189]
["8.63","High",11190]
["8.64","Medium",11191]
["8.65","Low",11192]
["8.66","High",11193]
["8.67","High",11194]
["8.68","High",11195]
["8.69","Medium",11196]
["8.7","High",8575]
["8.70","Medium",11197]
["8.71","Very High",11198]
["8.72","Medium",11199]
["8.73","Medium",11200]
["8.74","High",11201]
["8.75","Medium",11202]
["8.76","Medium",11203]
["8.77","Medium",11204]
["8.78","Medium",11205]
["8.79","Medium",11206]
["8.8","Medium",8576]
["8.80","Medium",11207]
["8.81","Low",11208]
["8.82","Medium",11209]
["8.83","Low",11210]
["8.84","Low",11211]
["8.85","Medium",11212]
["8.86","Medium",11213]
["8.87","Medium",11214]
["8.88","Low",11215]
["8.89","High",11216]
["8.9","High",8577]
["8.90","High",11217]
["8.91","High",11218]
["8.92","Medium",11219]
["8.93","Low",11220]
["8.94","Low",11221]
["8.95","Medium",11222]
["8.96","Medium",11223]
["8.97","Low",11224]
["8.98","High",11225]
["8.99","Medium",11226]
["9.1","Low",8390]
["9.10","Medium",8399]
["9.11","Medium",8400]
["9.12","Medium",8401]
["9.13","Low",8402]
["9.14","Medium",8403]
["9.15","Medium",8404]
["9.16","High",8405]
["9.17","High",8406]
["9.18","Low",8407]
["9.19","Low",8408]
["9.2","Very High",8391]
["9.20","Medium",8409]
["9.21","Medium",8410]
["9.22","Low",8411]
["9.23","Low",8412]
["9.24","Medium",8413]
["9.25","Low",8414]
["9.26","Low",8415]
["9.27","Low",8416]
["9.28","Medium",8417]
["9.29","Low",8418]
["9.3","Very High",8392]
["9.4","High",8393]
["9.5","High",8394]
["9.6","Low",8395]
["9.7","Medium",8396]
["9.8","Medium",8397]
["9.9","Medium",8398]
["9.99","High",8419]

{"sheet":"Equipment_list","index":7,"n_rows":21,"n_cols":3,"rows_kept":21,"cut":false,"hidden":true,"merged":[]}
["TITLE","Equipment_list_description","ID"]
["Accommodation ",null,12]
["Air Comp.",null,8]
["Aux. Engine",null,4]
["Aux. Mach.",null,7]
["Boiler",null,5]
["Cargo Mach.",null,13]
["Critical Equip.",null,16]
["Deck Mach.",null,18]
["Deck Pipe / Fittings",null,20]
["Documentation",null,21]
["Elect. Mach. & Equip.",null,10]
["Hull & Tanks",null,19]
["Inert Gas",null,14]
["LSA / FFA",null,17]
["Main Engine ",null,3]
["Miscellaneous",null,22]
["Nav & comm. equip.",null,11]
["ER Pipes, valves & fittings",null,9]
["Purifier",null,6]
["Mooring Mach.",null,15]

{"sheet":"PSC_MOU","index":8,"n_rows":11,"n_cols":3,"rows_kept":11,"cut":false,"hidden":true,"merged":[]}
["TITLE","PSC_MOU_description","ID"]
["Asia and the Pacific",null,2]
["Caribbean",null,4]
["Europe and the North Atlantic",null,1]
["Latin America",null,3]
["The Black Sea region",null,6]
["The Indian Ocean",null,8]
["The Mediterranean",null,7]
["The Riyadh MoU",null,9]
["USCG",null,10]
["West and Central Africa",null,5]

{"sheet":"Inspection_type","index":9,"n_rows":16,"n_cols":2,"rows_kept":16,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Bunkering Audit",14]
["Others (Eg. Insurance etc.)",12]
["Engineering Audit",16]
["Flag State Insp.",5]
["Ship Staff Insp.",15]
["IT Audit",10]
["OM Insp. (Eg. SIRE, CDI etc.)",6]
["ISM Audit",2]
["ISPS Audit",3]
["MLC Audit",1]
["Mooring Audit",9]
["Nav Audit / Verification",8]
["PSC Inspection",4]
["Suptd. Insp.",13]
["Terminal Insp.",11]

{"sheet":"Deficiency_Cause","index":10,"n_rows":8,"n_cols":3,"rows_kept":8,"cut":false,"hidden":true,"merged":[]}
["TITLE","Deficiency_Cause_description","ID"]
["Behaviour Based",null,1]
["Equipment Related",null,4]
["External Factors",null,5]
["Human Error",null,7]
["Inappropriate Procedure",null,8]
["Industry Issue",null,6]
["Knowledge Based",null,3]

{"sheet":"Observer_code","index":11,"n_rows":9,"n_cols":3,"rows_kept":9,"cut":false,"hidden":true,"merged":[]}
["TITLE","Observer_code_description","ID"]
["Class Surveyor",null,4]
["Others (Eg. Insurance etc.)",null,9]
["FSC Inspector",null,5]
["Owner / Marine / Tech. Suptd.",null,3]
["PSC Insp.",null,6]
["Ship Staff",null,2]
["SIRE / CDI Insp.",null,8]
["Terminal Insp.",null,7]

{"sheet":"Status_code","index":12,"n_rows":6,"n_cols":3,"rows_kept":6,"cut":false,"hidden":true,"merged":[]}
["TITLE","Status_code_description","ID"]
["Completed",null,6]
["Deferred to D D",null,5]
["In progress",null,3]
["Not Started",null,2]
["Waiting spare",null,4]

{"sheet":"PSC_ref_no","index":13,"n_rows":19,"n_cols":2,"rows_kept":19,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Alarms",9]
["Cargo operations including equipment",7]
["Certificates & Documentation",2]
["Dangerous Goods",13]
["Emergency Systems",5]
["Fire safety",8]
["ISM",16]
["ISPS",17]
["Life saving appliances",12]
["MLC, 2006",18]
["Other",19]
["Pollution Prevention",15]
["Propulsion and auxiliary machinery",14]
["Radio communication",6]
["Safety of Navigation",11]
["Structural condition",3]
["Water/Weathertight condition",4]
["Working and Living Conditions",10]

{"sheet":"Risk_value_of_obs","index":14,"n_rows":1,"n_cols":2,"rows_kept":1,"cut":false,"hidden":true,"merged":[]}
["Risk Value of observation","ID"]

{"sheet":"Year","index":15,"n_rows":18,"n_cols":1,"rows_kept":18,"cut":false,"hidden":true,"merged":[]}
["Year"]
[2014]
[2015]
[2016]
[2017]
[2018]
[2019]
[2020]
[2021]
[2022]
[2023]
[2024]
[2025]
[2026]
[2027]
[2028]
[2029]
[2030]

{"sheet":"Month","index":16,"n_rows":13,"n_cols":1,"rows_kept":13,"cut":false,"hidden":true,"merged":[]}
["Month"]
["Jan"]
["Feb"]
["Mar"]
["Apr"]
["May"]
["Jun"]
["Jul"]
["Aug"]
["Sep"]
["Oct"]
["Nov"]
["Dec"]

{"sheet":"Date_","index":17,"n_rows":32,"n_cols":1,"rows_kept":32,"cut":false,"hidden":true,"merged":[]}
["Date"]
["01"]
["02"]
["03"]
["04"]
["05"]
["06"]
["07"]
["08"]
["09"]
[10]
[11]
[12]
[13]
[14]
[15]
[16]
[17]
[18]
[19]
[20]
[21]
[22]
[23]
[24]
[25]
[26]
[27]
[28]
[29]
[30]
[31]

{"sheet":"Sheet1","index":18,"n_rows":24,"n_cols":6,"rows_kept":24,"cut":false,"hidden":true,"merged":[]}
[]
[null,"ID","E",null,"Date Recorded",1]
[null,"UNIQUE ID","F",null,"Type of Deficiency",2]
[1,"Date Recorded","G",null,"Observer code",3]
["ignore","Vessel Type","H",null,"Type of Inspection",4]
[null,"Internal / External","I",null,"Description of Deficiency",5]
[null,"Drydock","J",null,"Equipment Categories",6]
[null,"Information Sharing","K",null,"Area of Observation",7]
[null,"Critical_item","L",null,"Deficiency Cause",8]
[null,"Deficiency Type","M",null,"VIQ Ref Number",9]
[null,"Deficiency Cause","N",null,"Risk Value of Obs",10]
[null,"Inspection Type","O",null,"PSC Ref Number",11]
[null,"Equipments","P",null,"PSC MOU ID",12]
[null,"VIQ Reference Number","Q",null,"Action Taken or Required",13]
[null,"Risk Value of the observation","R",null,"Target Date",14]
[null,"PSC Reference Number","S",null,"PO Ref No.",15]
[null,"PSC MOU","T",null,"Status Code",16]
[null,"Observer Code","U",null,"Date Completed",17]
[null,"Target Date","V",null,"Drydock",18]
[null,"Status Code","W",null,"Info Sharing",19]
[null,"Description of Deficiency","X",null,"Critical Item Flag",20]
[null,"Action taken / required","Y",null,"Audit Type",21]
[null,"PO ref no","Z"]
[null,"Date completed","AA"]

{"sheet":"Ship_information","index":19,"n_rows":2,"n_cols":3,"rows_kept":2,"cut":false,"hidden":true,"merged":[]}
["Ship_ID","Ship_Name","FILE_NAME"]
["49","RESPECT (05-11-2019)","49_1576771650328.xlsm"]