{"text_format":"1","workbook":"xlsx","n_sheets":24,"sheets":["Mainsheet","Completed","Calc","Areaofobs","Vessel_type","Deficiency_type","VIQrefno","Equipment_list","PSC_MOU","Inspection_type","Deficiency_Cause","Observer_code","Status_code","PSC_ref_no","Risk_value_of_obs","Year","Month","Date_","Sheet1","Ship_information","External_Deficiency_type","External_Inspection_type","External_Observer_code","Sheet Version"],"not_rendered":{"charts":0,"images":5,"macros":1,"external_links":0,"defined_names":12,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Mainsheet","index":0,"n_rows":36,"n_cols":28,"rows_kept":36,"cut":false,"hidden":false,"merged":[[10,8,10,9],[10,12,10,13],[12,6,12,27],[8,6,8,27]]}
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,"Defect - Damage Monitoring Sheet"]
[]
[null,null,null,null,null,null,null,"Date of Report","31-Dec-2019",null,null,"Ship Name","DHT LOTUS (26-12-2019)"]
[]
[null,null,null,null,null,null,"VERSION : 2.0"]
[]
[]
[]
[null,null,null,null,"ID","UNIQUE ID","Date Recorded","Type of Deficiency","Observer code","Type of Inspection","Description of Deficiency","Equipment Categories","Area of Observation","Deficiency Cause","VIQ Ref Number","Risk Value of Obs","PSC Ref Number","PSC MOU ID","Action Taken or Required","Target Date","PO Ref No.","Status Code","Date Completed","Drydock","Info Sharing","Critical Item","Audit Type","Superintendent Remarks"]
[null,null,null,null,2548,"27_15/10/2019 8:26:56 AM","2019-02-20","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Purifier temperature control valves not functioning in Auto mode","E/R - Purifier","Eng. / Strg. Comp.","Equipment Related","","","","","to investigate and spares to order/ spares requisition raised","2019-03-31","DLOT190064","Waiting spare",null,"No","No","No","Internal"]
[null,null,null,null,2549,"27_15/10/2019 8:33:47 AM","2019-02-20","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","DG # 1 oilmax pump leaking ","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Have to overhaul","2019-03-30","DLOT190074","Not Started",null,"No","No","No","Internal"]
[null,null,null,null,9056,"27_Mon Nov 11 2019 18:39:37 GMT+0000 (Coordinated Universal Time)","2019-11-06","Other","Ship Staff","Ship Staff Insp.","Aux blr.no.1 flaming out intermittently.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","Fault traced with the flame sensor and flame scanner.Awaiting spares.","2019-12-05","DLOT190240 APPLIES","Waiting spare",null,"No","No","No","Internal"]
[null,null,null,null,9057,"27_15/11/2019 11:03:07 AM","2019-11-06","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","1S COT Temperature Sensor showing no readout","Miscellaneous","Cargo / Ballast Systems","Equipment Related","","","","","Sensor checked-Ok.Communication troubleshooting  in progress","2019-11-30","","In progress",null,"No","No","No","Internal"]
[null,null,null,null,9058,"27_15/11/2019 11:04:43 AM","2019-11-06","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","No.1 & No.3 COP Vibration Sensor Showing Erratic Readings while stopped","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","Awaiting Spares","2019-11-21","DLOT 190230","Waiting spare",null,"No","No","No","Internal"]
[null,null,null,null,9059,"27_15/11/2019 2:16:56 PM","2019-11-06","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Fireman radios were located on the bridge. Suggest they may be relocated near fireman's locker.","LSA / FFA","LSA / FFA Appliances","Knowledge Based","","","","","To relocate","2019-11-30","","Not Started",null,"No","No","No","Internal"]
[null,null,null,null,9060,"27_15/11/2019 2:19:04 PM","2019-11-06","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","PORT & STBD lifeboats' hook does not have indication/marking for open/shut","LSA / FFA","LSA / FFA Appliances","Inappropriate Procedure","","","","","To be marked","2019-11-30","","Not Started",null,"No","No","No","Internal"]
[null,null,null,null,9061,"27_15/11/2019 4:37:08 PM","2019-11-06","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ME - RPM indicator at local manoeuvring platform has an error of 10 rpm. When M/E was in STOP condition it is showing 10 RPM AHEAD.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related",null,null,"Not Applicable","Not Applicable","To be rectified","2019-11-15",null,"Not Started",null,"No","No","No","Internal"]
[null,null,null,null,9062,"27_16/11/2019 06:24:10","2019-11-06","Critical Equipment,Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Draft Gauge in CCR not Working","Miscellaneous","Cargo / Ballast Systems","Equipment Related",null,null,"Not Applicable","Not Applicable","Awaiting new I/O unit ","2019-11-30",null,"Waiting spare",null,"No","No","No","Internal"]
[null,null,null,null,9063,"27_16/11/2019 06:25:31","2019-11-06","Critical Equipment,Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Stripper Pump Stroke Counter showing Erratic Readings","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","Troubleshooting to be carried out","2019-11-30","","Not Started",null,"No","No","No","Internal"]
[null,null,null,null,9064,"27_16/11/2019 06:28:10","2019-11-06","Critical Equipment,Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","WBT Gas Detection System flow Sensor Fault","Critical Equip.","Cargo / Ballast Systems","Equipment Related","","","","","Troubleshooting carried out.New Sensor Installed.Flow Fail alarm still persists.Suspect problem with Mist Detector.Technicians to attend in Singpaore on 18 Nov 2019","2019-11-30","","In progress",null,"No","No","No","Internal"]
[null,null,null,null,9065,"27_16/11/2019 06:30:01","2019-11-06","Critical Equipment,Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","2nd Hydraulic Pump does not cut in on pressure drop in the system ","Critical Equip.","Cargo / Ballast Systems","Equipment Related","","","","","Troubleshooting to be carried out","2019-11-30","","Not Started",null,"No","No","No","Internal"]
[null,null,null,null,9067,"27_16/11/2019 07:13:27","2019-11-06","Critical Equipment,Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Phones in Accomodation had missing buttons on the dialing panel","Critical Equip.,Navigation - GMDSS & Communication","Communication","Behaviour Based,Human Error","","","","","To be attended & repaired","2019-11-30","DLOT190257","In progress",null,"No","No","No","Internal"]
[null,null,null,null,9069,"27_16/11/2019 10:22:10 AM","2019-11-06","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","SAAB alarm in the CCR is not audible. The volume intensity to be increased.","Elect. Mach. & Equip.","Cargo / Ballast Systems","Equipment Related",null,null,"Not Applicable","Not Applicable","To be rectified","2020-01-31",null,"Not Started",null,"No","No","No","Internal"]
[null,null,null,null,null,"27_05/01/2020 4:29:16 PM","2020-01-05","Observation","Ship Staff","Ship Staff Insp.","Capacitors  to disconnected/remove for the LED light fittings in the engine room and accomodation","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related",null,null,"Not Applicable","Not Applicable","Capacitors needs to be removed","2020-03-31",null,"In progress",null,"No",null,null,"Internal"]
[null,null,null,null,null,"27_14/01/2020 10:00:04 AM","2020-01-10","Other","Ship Staff","Ship Staff Insp.","Harbour sea water pump leaking from the mechanical seal","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related",null,null,"Not Applicable","Not Applicable","Mech.seal needs to be renewed","2020-04-09",null,"Not Started",null,"No",null,null,"Internal"]
[null,null,null,null,null,"27_14/01/2020 10:05:54 AM","2020-01-11","Other","Ship Staff","Ship Staff Insp.","Exhaust gas scrubber sea water pump no.3 mech.seal passing","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related",null,null,"Not Applicable","Not Applicable","Mech.seal needs renewal","2020-04-10",null,"Not Started",null,"No",null,null,"Internal"]
[null,null,null,null,null,"27_14/01/2020 10:08:30 AM","2020-01-11","Other","Ship Staff","Ship Staff Insp.","IGS Scrubber pump mech.seal leaking","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related",null,null,"Not Applicable","Not Applicable","Mech.seal needs renewal","2020-04-11",null,"Not Started",null,"No",null,null,"Internal"]
[null,null,null,null,null,"27_14/01/2020 11:01:44 AM","2020-01-12","Other","Ship Staff","Ship Staff Insp.","IGS Deck seal pump no.1 mech.seal leaking","Inert Gas","Eng. / Strg. Comp.","Equipment Related",null,null,"Not Applicable","Not Applicable","Mech.seal leaking due muddy water.Will replace seal.","2020-04-11",null,"Not Started",null,"No",null,null,"Internal"]

{"sheet":"Completed","index":1,"n_rows":199,"n_cols":28,"rows_kept":199,"cut":false,"hidden":false,"merged":[[10,8,10,9],[10,12,10,13],[12,6,12,27],[8,6,8,27]]}
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,"Defect - Damage Monitoring Sheet"]
[]
[null,null,null,null,null,null,null,"Date of Report","31-11-2019",null,null,"Ship Name","DHT LOTUS (26-12-2019)"]
[]
[null,null,null,null,null,null,"VERSION : 2.0"]
[]
[]
[]
[null,null,null,null,"ID","UNIQUE ID","Date Recorded","Type of Deficiency","Observer code","Type of Inspection","Description of Deficiency","Equipment Categories","Area of Observation","Deficiency Cause","VIQ Ref Number","Risk Value of Obs","PSC Ref Number","PSC MOU ID","Action Taken or Required","Target Date","PO Ref No.","Status Code","Date Completed","Drydock","Info Sharing","Critical Item","Audit Type","Superintendent Remarks"]
[null,null,null,null,2547,"27_15/10/2019 8:18:03 AM","2019-01-11","Defect","Ship Staff","Ship Staff Insp.","Air con compressor #1 oil return chamber float broken","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","Presently functioning satisfactory.","2019-02-28","","Completed","2019-12-24","No","No","No","Internal"]
[null,null,null,null,2550,"27_15/10/2019 8:35:57 AM","2019-02-20","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Oil leakage observed from Aft of local manoeuvring platform, source to be identified\t","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Oil leaks rectified.","2019-07-31","","Completed","2019-11-18","No","No","No","Internal"]
[null,null,null,null,2551,"27_15/10/2019 9:01:27 AM","2019-04-27","Defect","Ship Staff","Ship Staff Insp.","Aft Hydraulic storage tank gauge glass leaking","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","Leakage rectified by renewing the o-rings.","2019-07-30","","Completed","2019-11-27","No","No","No","Internal"]
[null,null,null,null,2552,"27_15/10/2019 9:04:55 AM","2019-04-27","Defect","Ship Staff","Ship Staff Insp.","DG lube oil settling and service tanks gauge glasses leaking.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","Gauge glass leakage rectified by replacing the o-rings.","2019-07-30","","Completed","2019-11-26","No","No","No","Internal"]
[null,null,null,null,2553,"27_15/10/2019 9:18:29 AM","2019-05-10","Defect","Ship Staff","Ship Staff Insp.","Cylinder oil daily tank gauge glass leaking from bottom valve","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","Top and bottom valve o-rings renewed","2019-08-15","","Completed","2019-11-26","No","No","No","Internal"]
[null,null,null,null,2554,"27_15/10/2019 9:25:20 AM","2019-06-01","Defect","Ship Staff","Ship Staff Insp.","44OV low Insulation  from ICO Lube power panel,Micromaster siemens.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","As per the e-mail from lukoil ,V/L to keep Icolub swiched off when not in operation,otherwise,to buy a transformer from them to put in E/E.","2019-09-01","","Completed","2019-12-12","No","No","No","Internal"]
[null,null,null,null,2555,"27_15/10/2019 14:30:50","2019-01-03","Defect","Ship Staff","Ship Staff Insp.","GALLEY COOKING RANGE INSULATION FAULT ","Accommodation","General Appearance","Equipment Related","5.25","Medium","","","HOT PLATE REPLACED WITH A SPARE ONE- OPERATING SATISFACTORY.","2019-12-31","","Completed","2019-11-12","No","No","No","Internal"]
[null,null,null,null,2556,"27_15/10/2019 14:34:16","2019-01-14","Defect,Other","Ship Staff","Ship Staff Insp.","NIGHT VISION BINOCULARS NON FUNCTIONAL ","Navigation - Others","Navigation","Equipment Related","7.4","Low","","","NEW  BINOCULARS RECEIVED","2019-12-31","","Completed","2019-04-04","No","No","No","Internal"]
[null,null,null,null,2557,"27_15/10/2019 14:38:57","2019-02-04","Defect","Ship Staff","Ship Staff Insp.","DECK SEAL OVERBOARD LINE INBOARD VALVE LEAKING FROM FLANGE IN PUMPROOM PORT SIDE ","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.27","Medium","","","VALVE REPLACED-NO LEAKS OBSERVED. ","2019-12-31","","Completed","2019-09-05","No","No","No","Internal"]
[null,null,null,null,2558,"27_15/10/2019 14:40:44","2019-02-04","Defect","Ship Staff","Ship Staff Insp.","CARGO VALVE CAV 188 ACTUATOR LEAKING ","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.44","High","","","ACTUATOR REPLACED-NO LEAKS OBSERVED","2019-12-30","","Completed","2019-09-05","No","No","No","Internal"]
[null,null,null,null,2559,"27_15/10/2019 14:44:29","2019-02-04","Defect","Ship Staff","Ship Staff Insp.","PLATFORM FOR CHANGING LIGHT IN PUMP ROOM UPPR PLATFORM NOT FITTED WITH GUARD RAILS ","LSA / FFA","LSA / FFA Appliances","Equipment Related","","","","","GUARD RAILS FITTED IN YULIAN SHIPYARD.","2019-12-31","","Completed","2019-09-09","No","No","No","Internal"]
[null,null,null,null,2560,"27_15/10/2019 14:48:02","2019-01-04","Defect","Ship Staff","OM Insp. (Eg. SIRE / CDI etc.)","MOORING WINCH TO BE DE RUSTED AND PAINTED ","Deck - Mooring Machinery","Cargo / Ballast Systems","Equipment Related","9.14","Medium","","","ALL MOORING WINCHES RUSTED AND PAINTED","2019-12-31","","Completed","2019-11-04","No","No","No","Internal"]
[null,null,null,null,2561,"27_15/10/2019 8:23:15 AM","2019-01-20","Defect","Ship Staff","Ship Staff Insp.","LP circulating pump #1 not operational","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","pump opened up found bearing bush damaged need overhaul spares ordered","2019-02-10","DLOT190071","Completed","2019-08-06","No","No","No","Internal"]
[null,null,null,null,2562,"27_15/10/2019 8:29:51 AM","2019-02-20","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Exhaust leakage observed from by-pass damper shaft bearings","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","valve to inspect and bearing to renew","2019-05-31","","Completed","2019-08-08","No","No","No","Internal"]
[null,null,null,null,2563,"27_15/10/2019 8:39:09 AM","2019-02-20","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ME LO auto backwash filter not turning","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.7","Medium","","","Spares received. Filters opened up and cleaned hydraulic unit motors and spares renewed","2019-04-30","DLOT190079","Completed","2019-08-14","No","No","No","Internal"]
[null,null,null,null,2564,"27_15/10/2019 8:41:52 AM","2019-03-18","Defect","Ship Staff","Ship Staff Insp.","Aft LT cooler sea water inlet pipe holed.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Temporary repair carried out with Devcon, pipe to be removed and renewed or welded repair carried out.\n\nDD spec raised for same in REFMAN.\n\n","2019-04-30","","Completed","2019-08-26","Yes","No","No","Internal"]
[null,null,null,null,2565,"27_15/10/2019 9:11:01 AM","2019-04-27","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","#1 & #3 Main Feed water pumps disch gauges needle found broken. ","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.31","Very High","","","vessel needs to order the pressure gauge 0- 40 bar in next store.","2019-07-27","","Completed","2019-09-22","No","No","No","Internal"]
[null,null,null,null,2566,"27_15/10/2019 9:14:19 AM","2019-05-02","Defect","Ship Staff","Ship Staff Insp.","Deck Seal - Pnuematic vent valve to atmosphere not-operational","Inert Gas","Cargo / Ballast Systems","Equipment Related","","","","","Trobleshooting in progress. Requisition to be raised for spares.","2019-08-01","","Completed","2019-08-08","No","No","No","Internal"]
[null,null,null,null,2567,"27_15/10/2019 9:22:23 AM","2019-05-15","Defect","Ship Staff","Ship Staff Insp.","Aft ICCP display not working","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","Troubleshooting carried out, input power available to PCB, concluded display defective, RO raised","2019-08-14","DLOT190111","Completed","2019-09-22","No","No","No","Internal"]
[null,null,null,null,2568,"27_15/10/2019 9:30:45 AM","2019-06-07","Defect","Ship Staff","Ship Staff Insp.","Fog local fire fighting system Battery Fault.","Elect. Mach. & Equip.","LSA / FFA Appliances","Equipment Related","","","","","Full system renewed","2019-09-07","","Completed","2019-09-10","No","No","No","Internal"]
[null,null,null,null,2569,"27_15/10/2019 10:15:11 AM","2019-06-15","Defect","Ship Staff","Ship Staff Insp.","Low sea chest suction valve remote operation hydralic leakage","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.31","Very High","","","During isolation for sea suction strainer cleaning the valve operated from remote hydralic system, found heavy oil leakage in the valve spindle , due to that valve is not closing fully.Vessel dont have manual for this particular valve to order any seals. Presently local manual operating hand wheel engaged and can operate manually from local position. valve need to be overhaul during drydock","2019-09-15","","Completed","2019-08-25","Yes","No","No","Internal"]
[null,null,null,null,2570,"27_15/10/2019 10:17:53 AM","2019-06-19","Defect","Ship Staff","Ship Staff Insp.","AE no.2 air cooler holding bolts seized in place","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Vessel planned for aircooler cleaning for no.2 aux engine. During opening found all the bolts are very hard to open, somehow managed to open the bolts except 2 pieces, which is seized in place. 2 bolts which is located inside the air intlet piece also found seized. various attempts made to open the seized bolts but couldn't succeed","2019-09-19","","Completed","2019-09-01","Yes","No","No","Internal"]
[null,null,null,null,2571,"27_15/10/2019 10:19:22 AM","2019-07-01","Defect","Ship Staff","Ship Staff Insp.","No.1HFO service tank heating coil outlet steam trap leaking","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Steam trap has to be overhauled","2019-10-01","","Completed","2019-08-16","No","No","No","Internal"]
[null,null,null,null,2572,"27_15/10/2019 10:21:39 AM","2019-07-02","Defect","Ship Staff","Ship Staff Insp.","FWD LT cooler S.W outlet pipe reducer leaking","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Temporary repairs carried out, leak arrested, need to renew the pipe at suitable opportunity","2019-10-02","","Completed","2019-08-26","No","No","No","Internal"]
[null,null,null,null,2573,"27_15/10/2019 10:23:52 AM","2019-07-02","Defect","Ship Staff","Ship Staff Insp.","COPT vaccum condenser bypass valve body get holed and leaking","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","8.33","Medium","","","Temporary repair carried out, leakage minimised, need to renew the valve","2019-10-02","","Completed","2019-08-16","No","No","No","Internal"]
[null,null,null,null,2574,"27_15/10/2019 10:27:26 AM","2019-07-03","Defect","Ship Staff","Ship Staff Insp.","COPT vaccum condensor S.W inlet pipe leaking","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","8.33","Medium","","","Temporary repair carried out, pipe section needs to be renewed","2019-10-03","","Completed","2019-08-16","No","No","No","Internal"]
[null,null,null,null,2575,"27_15/10/2019 10:29:43 AM","2019-07-03","Defect","Ship Staff","Ship Staff Insp.","All 3 COPT LO cooler oil side leaking","Cargo Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Cooler has to be inspected and packing need to be renewed during docking","2019-10-03","","Completed","2019-09-02","No","No","No","Internal"]
[null,null,null,null,2576,"27_15/10/2019 13:34:34","2019-01-06","Defect","Ship Staff","Ship Staff Insp.","LIFE BOAT DOOR HOLDER ARRANGEMENT DAMAGED ","LSA / FFA","LSA / FFA Appliances","Equipment Related","5.27","Medium","","","REPAIRS CARRIED OUT ","2019-01-15","","Completed","2019-01-07","No","No","No","Internal"]
[null,null,null,null,2577,"27_15/10/2019 13:47:36","2019-01-09","Defect","Ship Staff","Ship Staff Insp.","ONE OF THE COW LINE U CLAMP WAS MISSING ","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.34","High","","","NEW U CLAMP FITTED ","2019-02-12","","Completed","2019-01-09","No","No","No","Internal"]
[null,null,null,null,2578,"27_15/10/2019 13:50:50","2019-01-06","Defect","Ship Staff","Ship Staff Insp.","SIGHT GLASSES OF BOTH HOSE HANDLING CRANES DAMAGED / PAINTED OVER & NOT CLEAR ","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.63","High","","","ALL SIGHT GLASSES RENEWED ","2019-01-18","","Completed","2019-01-13","No","No","No","Internal"]
[null,null,null,null,2579,"27_15/10/2019 13:55:00","2019-01-12","Defect","Ship Staff","Ship Staff Insp.","W2 INOARD WINCH - WIRE END SECURING PLATE ALONG WITH STUD BOLTS DAMAGED DURING TRANSFERING OF WIRE ","Deck - Mooring Machinery","Mooring","Equipment Related","9.14","Medium","","","NEW P- PLATE ALONG WITH STUD BOLTS RENEWED & FITTED TO W2 DRUM PLATE ","2019-01-13","","Completed","2019-01-13","No","No","No","Internal"]
[null,null,null,null,2580,"27_15/10/2019 13:59:22","2019-01-13","Defect","Ship Staff","Ship Staff Insp.","WIRE LASHING OF SECURING PIPES NOT FOUND ON PORT FUNNEL DECK WERE FOUND PARTLY DAMAGED DUE TO CORRISION ","Deck - Machinery","General Appearance","Equipment Related","5.11","Low","","","LASHING RENEWED ","2019-01-15","","Completed","2019-01-13","No","No","No","Internal"]
[null,null,null,null,2581,"27_15/10/2019 14:02:06","2019-01-12","Defect","Ship Staff","Ship Staff Insp.","ALL 4 VECS MANIFOLD 12 CLOCK POSITION STUD BOLTS FOUND WASTED ","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","","","","","ALL 4 RENEWED ","2019-01-19","","Completed","2019-01-14","No","No","No","Internal"]
[null,null,null,null,2582,"27_15/10/2019 14:05:06","2019-01-14","Defect","Ship Staff","Ship Staff Insp.","1 FOAM LINE & FIRE LINE DRESSOR COUPLING FOUND LEAKING ","LSA / FFA","LSA / FFA Appliances","External Factors","","","","","WEDGE RINGS RENEWED .LEAK ARRESTED ","2019-01-20","","Completed","2019-01-15","No","No","No","Internal"]
[null,null,null,null,2583,"27_15/10/2019 14:18:47","2019-01-16","Defect","Ship Staff","Ship Staff Insp.","OFFICER MESS ROOM VENT FLAP RETAINING CHANNEL FOUND DAMAGED ","Accommodation ,Deck - Machinery","General Appearance","Equipment Related","11.13","Low","","","SAME FABRICATED AND RUBBER PACKING RENEWED ","2019-01-19","","Completed","2019-01-17","No","No","No","Internal"]
[null,null,null,null,2584,"27_15/10/2019 14:53:20","2019-03-21","Defect","Ship Staff","Ship Staff Insp.","MOORING WINCH M1 / M4 / M5 HYDRAULIC LEAK ","E/R - Boiler,Deck - Mooring Machinery","Mooring","Equipment Related","9.14","Medium","","","M4 AND M5 NEW BLOCK WITH ORINGS AND SHAFT RENEWED LEAKAGES RECTIFIED M1 HAS NO LEAKS ","2019-04-30","","Completed","2019-04-12","No","No","No","External"]
[null,null,null,null,2585,"27_15/10/2019 14:56:38","2019-04-20","Defect","Ship Staff","Ship Staff Insp.","FIRE AND GS PUMP MECHNICAL SEAL LEAKING ","LSA / FFA","LSA / FFA Appliances","Equipment Related","5.35","Medium","","","MECHNIACL SEAL RENEWED AT SUITABLE OPPORTUNITY ","2019-05-16","","Completed","2019-07-27","No","No","No","Internal"]
[null,null,null,null,2586,"27_15/10/2019 14:59:15","2019-03-30","Defect","Ship Staff","Ship Staff Insp.","NEW SLINGS , CHAIN BLOCKS AS PER SAFETY FLASH 81 TO BE PROCURED ","LSA / FFA","LSA / FFA Appliances","Equipment Related","5.11","Low","","","REQN RAISED / AWAITING SPARES ","2019-04-30","","Completed","2019-04-27","No","No","No","External"]
[null,null,null,null,5700,"27_29/10/2019 5:18:47 PM","2019-10-27","Defect","Ship Staff","Ship Staff Insp.","VENT FLAPS AT ECONOMISER LP PLATFORM & SCRUBBER ROOM TURNING VERY HARD","Miscellaneous","Emgcy. Systems","Equipment Related","","","","","VENT FLAPS REMOVED FROM PLACE,EASED UP IN THE W/SHOP AND BOXED BACK-SATISFACTORY","2019-10-30","","Completed","2019-10-27","No","No","No","Internal"]
[null,null,null,null,5701,"27_21/10/2019 4:24:18 PM","2019-10-21","Defect","Ship Staff","Ship Staff Insp.","EMG.GENERATOR ROOM STBD.SIDE VENT FLAP SEIZED","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","FlLAP VANES OBSERVED TO BE BADLY RUSTED,NEEDS TO BE CHIPPED AND PAINTED.ALL DONE-OPERATING SATIS.","2019-10-30","","Completed","2019-10-28","No","No","No","Internal"]
[null,null,null,null,5702,"27_29/10/2019 5:36:28 PM","2019-10-29","Defect","Ship Staff","Ship Staff Insp.","NO1 & NO.2 HFO SETT TANK O'FLOW PIPE GAUGE GLASS LEAKING","Deck - Pipe / Fittings","Eng. / Strg. Comp.","Equipment Related","","","","","GAUGE GLASS RENEWED WITH A SPARE ONE","2019-10-31","","Completed","2019-10-29","No","No","No","Internal"]
[null,null,null,null,5704,"27_21/10/2019 4:11:35 PM","2019-10-16","Defect","Ship Staff","Ship Staff Insp.","FAILURE OF AC-DC CONVERTER UNIT FOR  M/E RPLS","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","PSU UNIT REPLACED AND SYSTEM FOUND TO BE WORKING STAISFACTORY","2019-12-16","RO DLOT 190227 RAISED","Completed","2019-11-04","No","No","No","Internal"]
[null,null,null,null,5705,"27_29/10/2019 1:26:36 PM","2019-10-26","Guarantee Claim","Ship Staff","Ship Staff Insp.","SOX SCRUBBER FLOW METER DEFECTIVE","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","GUARANTEE SERVICE ENGR. ATTENDED THE V/L AT ULSAN AND REPLACED THE PCB BOARD INSIDE THE FLOWMETER CARTRIDGE-OPERATION SATISFACTORY","2019-12-25","","Completed","2019-11-06","No","No","No","Internal"]
[null,null,null,null,5706,"27_29/10/2019 5:31:35 PM","2019-10-28","Other","Ship Staff","Ship Staff Insp.","Erratic  PLC Controller of refrigeration control panel.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","Observed for more than a month and no problem experienced.","2019-12-25","","Completed","2019-12-07","No","No","No","Internal"]
[null,null,null,null,5707,"27_43779.653599537","2019-09-13","Critical Equipment","Ship Staff","Ship Staff Insp.","Fire alarm showing fault ","LSA / FFA","LSA / FFA Appliances","Equipment Related","5.35","Medium","","","smoke sensor and manual call point needed for attendence.Manual call point renewed and system is functioning satisfactory.","2019-10-30","DLO190178 and DLOT190210","Completed","2019-10-28","No","No","No","Internal"]
[null,null,null,null,9055,"27_16/11/2019 07:04:51","2019-11-06","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Strong Draft of air coming from side of AC Duct & Black stain was visible","Miscellaneous","Eng. / Strg. Comp.","Behaviour Based,Human Error","","","","","Black stain marks cleared.","2019-11-30","","Completed","2019-11-17","No","No","No","Internal"]
[null,null,null,null,9071,"27_Sun Aug 11 2019 11:06:24 GMT+0000 (Coordinated Universal Time)","2019-11-01","Defect","Ship Staff","Ship Staff Insp.","B/R MIDDLE WINDOW WIPER INOPERATIONAL.","Elect. Mach. & Equip.","Navigation","Equipment Related","","","","","COMLETE WIPER ASSY REMOVED FROM PLACE ,AND INSPECTED.OBERVED BELT GUIDE LOCKING BOLTS WORN OUT,SAME REPLACED AND WIPER FOUND TO OPERATING SATISFAC TORY.","2019-11-04","","Completed","2019-11-01","No","No","No","Internal"]
[null,null,null,null,9072,"27_Fri Oct 11 2019 19:54:37 GMT+0000 (Coordinated Universal Time)","2019-11-04","Breakdown","Ship Staff","Ship Staff Insp.","VECS sensor was damaged","Deck - Machinery","Cargo / Ballast Systems","Equipment Related","","","","","New sensor recevied and renewed ","2020-11-20","","Completed","2019-11-11","No","No","No","Internal"]
[null,null,null,null,9073,"27_Fri Oct 11 2019 19:59:28 GMT+0000 (Coordinated Universal Time)","2019-11-06","Breakdown","Ship Staff","Ship Staff Insp.","Flow sensor was not giving any output signal in ballast tank gas detection system","Hull & Tanks","Cargo / Ballast Systems","Equipment Related","","","","","Flow sensor, PCB board and Transformer was renwed with the spare","2019-11-20","","Completed","2019-11-10","No","No","No","Internal"]
[null,null,null,null,9074,"27_Mon Nov 11 2019 18:45:27 GMT+0000 (Coordinated Universal Time)","2019-11-08","","Ship Staff","Ship Staff Insp.","AHU NO.1 AND 2  FRESH AIR INTAKE FLAPS SEIZED AND OPERATING LINKAGE BROKEN","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","FLAPS MADE FREE AND LINKAGES REPAIRED","2019-11-10","","Completed","2019-11-08","No","No","No","Internal"]
[null,null,null,null,9075,"27_13/11/2019 10:34:55 AM","2019-11-08","Other","Ship Staff","Ship Staff Insp.","SCRUBBER PUMP OVERBOARD LINE LEAKING FROM THE WELD JOINT","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","CORRODED/WASTED PIPE (L-1000MM X NB-350MM|) RENEWED WITH A GALVANISED AND EPOXY COATED PIPE.","2019-11-15","","Completed","2019-11-12","No","No","No","Internal"]
[null,null,null,null,9076,"27_43779.6773032407","2019-10-02","Other","Ship Staff","Ship Staff Insp.","Anemometer in CCR is non functional ","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","5.9","Very High","","","RESTORED THE WINDOWS IN THE SYSTEM-FUNCTIONING SATISFACTORY.","2019-10-30","","Completed","2019-11-05","No","No","No","Internal"]
[null,null,null,null,9077,"27_Sun Nov 10 2019 16:25:11 GMT+0000 (Coordinated Universal Time)","2019-10-10","Other","Ship Staff","Ship Staff Insp.","Stbd Windlass brake assembly leaky due to scoring of rams ","Deck - Machinery,Deck - Mooring Machinery","Mooring","Equipment Related","9.14","Medium","","","SHAFT BUILD UP BELZONA AND SMOOTHENED.SEALS REPACED.","2019-10-30","","Completed","2019-11-01","No","No","No","Internal"]
[null,null,null,null,9078,"27_13/11/2019 11:07:48 AM","2019-11-08","Other","Ship Staff","Ship Staff Insp.","A/E2 CHARGE AIR TEMP.SENSOR GIVING ERRATIC READ OUT.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","SENSOR RENEWED - WORKING SATISFACTORY","2019-11-16","","Completed","2019-11-08","No","No","No","Internal"]
[null,null,null,null,9079,"27_13/11/2019 2:02:42 PM","2019-11-09","Breakdown","Ship Staff","Ship Staff Insp.","One of the limit switch in stbd side davit was not working, its contacts are damaged due the weather condition\t\t","Deck - Machinery","LSA / FFA Appliances","External Factors","","","","","Switch renewed with the spare one after repairing the base plate.","2019-11-16","","Completed","2019-11-10","No","No","No","Internal"]
[null,null,null,null,9080,"27_15/11/2019 05:19:50","2019-11-06","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Tiles in Ship's Laundry found Broken/Cracked/missing","Miscellaneous","General Appearance","External Factors","","","","","Old Broken/ Cracked tiles removed and area patched up with cement ","2019-11-06","","Completed","2019-11-06","No","No","No","Internal"]
[null,null,null,null,9081,"27_43779.6758912037","2019-09-26","Other","Ship Staff","Ship Staff Insp.","Pumproom gas detection system sensor non functional ","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.21","High","","","Pumproom Bottom Stbd HC Sensor Renewed","2019-11-30","dlot 190008","Completed","2019-11-14","No","No","No","Internal"]
[null,null,null,null,9082,"27_Fri Nov 08 2019 11:13:31 GMT+0000 (Coordinated Universal Time)","2019-11-01","Breakdown","Ship Staff","Ship Staff Insp.","PUMP RM HC SENSOR STBD SIDE NOT GIVING ANY OUTPUT DURING CALIBRATION","Elect. Mach. & Equip.","Cargo / Ballast Systems","Equipment Related","","","","","HC  SENSOR Pumproom Bottom Stbd Replaced.Zero & Span Gas Calibration Done","2019-11-08","","Completed","2019-11-14","No","No","No","Internal"]
[null,null,null,null,9083,"27_15/11/2019 05:28:38","2019-11-06","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Stbd Provision Crane Platform Door/Safety Barrier Wasted","Miscellaneous","General Appearance","Equipment Related","","","","","New Door/Safety Barrier Fabricated","2019-11-14","","Completed","2019-11-14","No","No","No","Internal"]
[null,null,null,null,9084,"27_15/11/2019 05:31:56","2019-11-06","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Stbd Manifolad Drip Tray Ladder Steps Wasted","Miscellaneous","Structural Condn. / WT integrity ","Equipment Related","","","","","2 New Steps Fabricated","2019-11-12","","Completed","2019-11-12","No","No","No","Internal"]
[null,null,null,null,9085,"27_15/11/2019 06:09:47","2019-11-06","Critical Equipment,Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Slop P Temperature Repeater on CCR Panel showing Error","Miscellaneous","Cargo / Ballast Systems","Equipment Related","","","","","Repeater Panel Connection Checked & Error Rectified","2019-11-10","","Completed","2019-11-10","No","No","No","Internal"]
[null,null,null,null,9086,"27_15/11/2019 11:14:21 AM","2019-11-06","Critical Equipment,Defect","Owner / Marine / Tech. Suptd.,SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","Minor leak in Hydraulic room from stack of hydraulic Lines","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","Hydraulic Pump Kept Running for 3 days .No evident leak observed.No appreciable change in Hydraulic Level.All Armato Couplings tightened.Hydraulic Lines under continuos monitoring.All Valves in Hydraulic Room operated one by one.","2019-11-15","","Completed","2019-11-14","No","No","No","Internal"]
[null,null,null,null,9087,"27_15/11/2019 11:22:18 AM","2019-11-06","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Cabin Washroom Floor & Curtain were found dirty & Sanitary fittings Leaking","Accommodation","MLC Related","Behaviour Based","","","","","Washroom Flooring Cleaned.Shower Curtains Renewed.Shower Fittings Renewed","2019-11-15","","Completed","2019-11-14","No","No","No","Internal"]
[null,null,null,null,9088,"27_15/11/2019 1:47:51 PM","2019-11-06","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","SMB starter panel located in fwd store has been decommissioned.","Deck - Machinery","General Appearance","Equipment Related","","","","","Marked.","2019-11-30","","Completed","2019-11-15","No","No","No","Internal"]
[null,null,null,null,9089,"27_15/11/2019 2:21:41 PM","2019-11-06","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","STBD side lifeboat - box for lifeboat winch hoisting is broken","LSA / FFA","LSA / FFA Appliances","Equipment Related","","","","","Box repaired.","2019-11-30","","Completed","2019-11-14","No","No","No","Internal"]
[null,null,null,null,9090,"27_15/11/2019 4:25:47 PM","2019-11-06","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","E/R - slight leak from one of the valves for the hot water tank/circulating pump","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Flange tightened and leakage rectified","2019-11-15","","Completed","2019-11-12","No","No","No","Internal"]
[null,null,null,null,9091,"27_15/11/2019 4:51:26 PM","2019-11-06","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","CCR - VECS system has a constant alarm 31. Loop, displayed.","Elect. Mach. & Equip.","Cargo / Ballast Systems","Equipment Related","","","","","Sensor Renewed.Fault rectified","2019-11-15","","Completed","2019-11-10","No","No","No","Internal"]
[null,null,null,null,9092,"27_15/11/2019 2:45:10 PM","2019-11-06","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Indicator plate for 1S COT IG valve is fitted in opposite direction","Cargo Mach.,Deck - Pipe / Fittings,Inert Gas","Cargo / Ballast Systems","Equipment Related","","","","","1S IG Valve Gear Renewed","2019-11-30","","Completed","2019-11-15","No","No","No","Internal"]
[null,null,null,null,9093,"27_15/11/2019 3:09:18 PM","2019-11-06","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Pumproom - last inspection date for the port side void space to be marked - located on deck above pumproom bottom","Miscellaneous","Cargo / Ballast Systems","Human Error,Inappropriate Procedure","","","","","Pumproom Void Space Inspected & new Date marked","2019-11-30","","Completed","2019-11-15","No","No","No","Internal"]
[null,null,null,null,9094,"27_15/11/2019 05:24:45","2019-11-06","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Weathertight Doors Channels Found Wasted - Deck Workshop/Steering Gear","Miscellaneous","Structural Condn. / WT integrity ","Equipment Related","","","","","New Channels fabricated","2019-11-16","","Completed","2019-11-15","No","No","No","Internal"]
[null,null,null,null,9095,"27_15/11/2019 1:52:00 PM","2019-11-06","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","STBD side midship store has lot of loose U clamps lying which can easily slip during rolling","Deck - Pipe / Fittings","General Appearance","Equipment Related","","","","","U-Bolts Secured.Battons in Place","2019-11-30","","Completed","2019-11-10","No","No","No","Internal"]
[null,null,null,null,9096,"27_15/11/2019 1:54:05 PM","2019-11-06","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","STBD side aft MARPOL line manifold has 2 reducers fitted","Deck - Pipe / Fittings","MARPOL Related","Equipment Related","","","","","Reducer Removed.Line Blanked","2019-11-30","","Completed","2019-11-12","No","No","No","Internal"]
[null,null,null,null,9097,"27_15/11/2019 2:29:34 PM","2019-11-06","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","SOPEP air diaphragm pump rigged at the break of accomodation was tried out and found an air leak at the connection between the flexible pipe and flexible piping.","Deck - Pipe / Fittings","MARPOL Related","Equipment Related","","","","","Leak Rectified.Rubber Packing for hose Coupling Renewed","2019-11-30","","Completed","2019-11-11","No","No","No","Internal"]
[null,null,null,null,9098,"27_15/11/2019 2:39:08 PM","2019-11-06","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Entrance to Incinerator room has been incorrectly marked as \"Garbage room\"","Miscellaneous","General Appearance","Human Error","","","","","Label Removed","2019-11-30","","Completed","2019-11-11","No","No","No","Internal"]
[null,null,null,null,9099,"27_15/11/2019 2:07:06 PM","2019-11-06","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","5S WBT sounding pipe's threads are wasted","Deck - Pipe / Fittings,Hull & Tanks","MARPOL Related","Equipment Related","","","","","New Threads made & greased.","2019-11-30","","Completed","2019-11-11","No","No","No","Internal"]
[null,null,null,null,9100,"27_15/11/2019 4:19:22 PM","2019-11-06","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Pumproom - EEBD storage box in the pump room bottom is not secured properly in pace and lying loose on the grating.","LSA / FFA","LSA / FFA Appliances","Human Error,Inappropriate Procedure","","","","","EEBD box Removed.EEBD secured on the hooks","2019-11-30","","Completed","2019-11-15","No","No","No","Internal"]
[null,null,null,null,9101,"27_15/11/2019 2:35:13 PM","2019-11-06","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","In paint store, cargo samples are stacked on top of each other and some containers are stowed above securing bars","Miscellaneous","MARPOL Related","Human Error,Inappropriate Procedure","","","","","Cargo Samples Secured & stowed below Securing Bars","2019-11-30","","Completed","2019-11-10","No","No","No","Internal"]
[null,null,null,null,9102,"27_15/11/2019 1:39:55 PM","2019-11-06","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","IG line - Mast riser - has one sighting port located on the aft piping - the retaining ring has one bolt missing.","Deck - Pipe / Fittings,Inert Gas","MARPOL Related","Equipment Related","","","","","New bolt in place","2019-11-30","","Completed","2019-11-14","No","No","No","Internal"]
[null,null,null,null,9103,"27_16/11/2019 06:40:46","2019-11-06","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Duty messroom Bulkheads found dirty with oil stains","Accommodation","General Appearance","Behaviour Based,Human Error","","","","","Bulkheads Cleaned","2019-11-15","","Completed","2019-11-13","No","No","No","Internal"]
[null,null,null,null,9104,"27_16/11/2019 07:20:21","2019-11-06","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Engine Room Workshop deck metal plated were not properly secured","Miscellaneous","Eng. / Strg. Comp.","Behaviour Based,Human Error","","","","","Plates secured properly at designated area.","2019-11-30","","Completed","2019-11-15","No","No","No","Internal"]
[null,null,null,null,9105,"27_16/11/2019 07:43:55","2019-11-06","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Floor plate for Hot Well outside ECR found with Soft Patches","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Behaviour Based,Human Error","","","","","Floor plate chipped off completely, freshly primered and painted.","2019-11-30","","Completed","2019-11-15","No","No","No","Internal"]
[null,null,null,null,9106,"27_16/11/2019 08:29:00","2019-11-06","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","One Sling strap was found hanging on an overhead pipe located near soot collecting Tank","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Behaviour Based,Human Error","","","","","Sling strap secured/removed.","2019-11-30","","Completed","2019-11-15","No","No","No","Internal"]
[null,null,null,null,9107,"27_16/11/2019 07:49:53","2019-10-06","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Earthing Wire for the flow meter for Scrubber line to be secured","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Behaviour Based,Human Error","","","","","Earthing Wire checked & Secured properly","2019-11-30","","Completed","2019-11-16","No","No","No","Internal"]
[null,null,null,null,9108,"27_16/11/2019 08:13:46","2019-11-06","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Control Panel for Gen. service & Control Air Compressor is Decommisioned.Same to be marked","Miscellaneous","Eng. / Strg. Comp.","Behaviour Based,Human Error","","","","","Unit has marked as decommisioned","2019-11-30","","Completed","2019-11-15","No","No","No","Internal"]
[null,null,null,null,9109,"27_16/11/2019 8:53:13 AM","2019-11-06","Critical Equipment","Ship Staff","Suptd. Insp.","Securing bolts are missing for 15ppm separator thermo control box\t","Critical Equip.","Emgcy. Systems","External Factors","","","","","Bolts secured","2019-11-20","","Completed","2019-11-16","No","No","No","Internal"]
[null,null,null,null,9110,"27_15/11/2019 11:17:58 AM","2019-11-06","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Securing Bolts /Studs for Scrubber Overboard Pipe threads not protruding out of securing nut.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related,Human Error","","","","","Bolts replaced with correct size and length  ","2019-11-30","","Completed","2019-11-20","No","No","No","Internal"]
[null,null,null,null,9111,"27_16/11/2019 07:09:34","2019-11-06","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Icing found on pipes & tank of No.2 AC Reefer Compressor Unit inside AC Room","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","Refer compressor discharge pressure increased by throttling the condenser cooling outlet valve.","2019-11-30","","Completed","2019-11-10","No","No","No","Internal"]
[null,null,null,null,9112,"27_16/11/2019 07:22:08","2019-11-06","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Leak observed form flange adjacent to Main Engine Lube oil Setling Tank Outlet Valve","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Flange bolts tightened.","2019-11-30","","Completed","2019-11-21","No","No","No","Internal"]
[null,null,null,null,9113,"27_15/11/2019 1:33:36 PM","2019-11-06","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Hydraulic leak from the STBD side windlass brake cylinder","Deck - Mooring Machinery","Mooring","Equipment Related","","","","","Brake cylinder top cover seal ring and dust seal renewed-no leaks observed.","2019-11-30","","Completed","2019-11-22","No","No","No","Internal"]
[null,null,null,null,9114,"27_16/11/2019 07:07:24","2019-11-06","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Vent in AC Room - all bolts were missing","Miscellaneous","Eng. / Strg. Comp.","Behaviour Based,Human Error","","","","","Vent Frame secured with new bolts","2019-11-30","","Completed","2019-11-20","No","No","No","Internal"]
[null,null,null,null,9115,"27_16/11/2019 07:23:37","2019-11-06","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Old Valves in Engine room were not secured properly","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Behaviour Based,Human Error","","","","","Old Valves properly secured with wire","2019-11-30","","Completed","2019-11-22","No","No","No","Internal"]
[null,null,null,null,9116,"27_16/11/2019 07:25:34","2019-11-06","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Flexible pipe from Port boiler found with oil stains below the outlet","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","No.1 boiler flexible hose stain marks cleaned -no leaks observed","2019-11-30","","Completed","2019-11-19","No","No","No","Internal"]
[null,null,null,null,9117,"27_16/11/2019 07:26:46","2019-11-06","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Drums in steering gear loosely secured","Miscellaneous","Eng. / Strg. Comp.","Behaviour Based,Human Error","","","","","Drums secured properly with wire.","2019-11-30","","Completed","2019-11-22","No","No","No","Internal"]
[null,null,null,null,9118,"27_16/11/2019 07:29:16","2019-11-06","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","No.2 Aux Boiler Isolating & adjacent Valves found with Insufficient Lagging","E/R - Boiler","Eng. / Strg. Comp.","Behaviour Based,Human Error","","","","","Sufficient lagging placed and secured in place.","2019-11-30","","Completed","2019-11-21","No","No","No","Internal"]
[null,null,null,null,9119,"27_16/11/2019 08:24:00","2019-11-06","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Mesh for Soot Collectin Tank Cover found broken & missing in sections.Cover found loose","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Behaviour Based,Human Error","","","","","Mesh renewed & secured","2019-11-30","","Completed","2019-11-21","No","No","No","Internal"]
[null,null,null,null,9120,"27_16/11/2019 08:30:55","2019-11-06","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Engine Room Tank Markings/Identification missing","Miscellaneous","Eng. / Strg. Comp.","Behaviour Based,Human Error","","","","","Stenciling done as required.","2019-11-30","","Completed","2019-11-20","No","No","No","Internal"]
[null,null,null,null,9121,"27_16/11/2019 08:32:48","2019-11-06","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Engine Room Bottom Platform - The connection between the deadweight & the pedestral for lifting was disconnected","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Behaviour Based,Human Error","","","","","Deadweight & pedestral  connected","2019-11-30","","Completed","2019-11-19","No","No","No","Internal"]
[null,null,null,null,9122,"27_16/11/2019 08:21:14","2019-11-06","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Fire Extinguisher in Engine Room near Scrubber Pipe to be relocated to an accessiblelocation","LSA / FFA","LSA / FFA Appliances","Behaviour Based,Human Error","","","","","Fire Extinguisher relocated.","2019-11-30","","Completed","2019-11-16","No","No","No","Internal"]
[null,null,null,null,9123,"27_16/11/2019 07:45:25","2019-11-06","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Manifold Cover located on platform below ECR port side was not secured","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Behaviour Based,Human Error","","","","","Covers secured with proper bolts","2019-11-30","","Completed","2019-11-21","No","No","No","Internal"]
[null,null,null,null,9124,"27_16/11/2019 07:36:22","2019-11-06","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Lagging found soaked in oil underneath the platform near new Aux Generator","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Behaviour Based,Human Error","","","","","Flange tightened,cleaned and lagging painted. ","2019-11-30","","Completed","2019-11-17","No","No","No","Internal"]
[null,null,null,null,9125,"27_16/11/2019 07:31:53","2019-11-06","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Valves in Engine room for Generators found leaking from gland packing","E/R - Aux. Mach.","Eng. / Strg. Comp.","Behaviour Based,Human Error","","","","","Gland packing tightened and no leaks observed.","2019-11-30","","Completed","2019-11-20","No","No","No","Internal"]
[null,null,null,null,9126,"27_15/11/2019 2:53:25 PM","2019-11-06","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","#2 COP - pumproom - slight oil leak from the casing bolts and upper seal","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","Bolts tightened and oil cleaned.","2019-11-29","","Completed","2019-11-22","No","No","No","Internal"]
[null,null,null,null,9127,"27_15/11/2019 05:15:47","2019-11-06","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Securing Latches for AC Filter Missing in few locations","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","New latches fabricated and fitted in place","2019-11-30","","Completed","2019-11-22","No","No","No","Internal"]
[null,null,null,null,9128,"27_15/11/2019 11:19:54 AM","2019-11-06","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","3 Securing Bolts missing on Cover box of 15 ppm Bilge Separator Thermos Control Box","Critical Equip.","Eng. / Strg. Comp.","Human Error","","","","","Bolts fixed & cover box secured","2019-11-18","","Completed","2019-11-17","No","No","No","Internal"]
[null,null,null,null,9129,"27_Sun Nov 10 2019 15:53:50 GMT+0000 (Coordinated Universal Time)","2019-09-18","Other","Ship Staff","Ship Staff Insp.","A/E no 3 crank case getting pressurized ","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","crankcase vent line newly fabricated to nominal dia 80A as per makers reccomendation","2019-12-31","dlot 190216","Completed","2019-11-17","No","No","No","Internal"]
[null,null,null,null,9130,"27_15/11/2019 4:34:43 PM","2019-11-06","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","E/R - slight leak from the gland of the aft draft gauge valve located on the aft STBD side at bottom platform","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","gland retightened, no traces of leak.","2019-12-15","","Completed","2019-11-06","No","No","No","Internal"]
[null,null,null,null,9131,"27_16/11/2019 07:48:30","2019-11-06","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Main Engine Cylinder Lubricating System ( RPLS pump) found leaking","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","bolts retightened, no more leaks.","2019-11-30","","Completed","2019-11-06","No","No","No","Internal"]
[null,null,null,null,9132,"27_Sun Nov 10 2019 15:58:11 GMT+0000 (Coordinated Universal Time)","2019-09-20","Other","Ship Staff","Ship Staff Insp.","LSMGO Main line manifold valve is not with gear operated ","Deck - Pipe / Fittings","Eng. / Strg. Comp.","Equipment Related","6.7","High","","","LSMGO main maniflod fitted with gear operated valves","2019-12-30","","Completed","2019-11-25","No","No","No","Internal"]
[null,null,null,null,9133,"27_15/11/2019 11:07:39 AM","2019-11-06","Critical Equipment,Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Air Leak in CCR IG Panel Cabinet","Inert Gas","Cargo / Ballast Systems","Equipment Related","","","","","Vent valve eased up and flow regulation adjusted for less purging of air","2019-11-30","","Completed","2019-11-22","No","No","No","Internal"]
[null,null,null,null,9134,"27_15/11/2019 4:23:34 PM","2019-11-06","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Steering gear room - Fireman locker needs proper securing arrangement\t","LSA / FFA","LSA / FFA Appliances","Equipment Related","","","","","Proper securing arrangement made","2019-12-15","","Completed","2019-11-26","No","No","No","Internal"]
[null,null,null,null,9135,"27_16/11/2019 06:37:41","2019-11-06","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Indicator Lamp for Hi-Hi & VECS panel Power Button not working","Miscellaneous","Cargo / Ballast Systems","Equipment Related","","","","","Indicator Lamp is working for Hi-Hi & VECS ppower panel.","2019-11-30","","Completed","2019-11-27","No","No","No","Internal"]
[null,null,null,null,9136,"27_15/11/2019 4:31:11 PM","2019-11-06","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","E/R - lower/upper plunger for the level indicator for some of the tanks was found in stuck position. E.g. EGB soot tank, hyd tank for aft mooring, hot well tank etc","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Gauge glass isolating valves eased up.","2019-12-31","","Completed","2019-11-27","No","No","No","Internal"]
[null,null,null,null,9137,"27_16/11/2019 07:18:47","2019-11-06","Critical Equipment,Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Open/Shut Indicator for Central Cooler B/V High Seachest / Low Seachest not Working","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Limit switches rebnewed-working satisfactory.","2019-11-30","","Completed","2019-11-22","No","No","No","Internal"]
[null,null,null,null,9138,"27_16/11/2019 10:30:51 AM","2019-11-06","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","CCR - The bulb for the power indicator for Hi-Hi level alarm panel is not working. As a result it cannot be made out if the panel is in or off.","Cargo Mach.,Elect. Mach. & Equip.","Cargo / Ballast Systems","Equipment Related","","","","","Power indicator lamp is working","2020-01-31","","Completed","2019-11-26","No","No","No","Internal"]
[null,null,null,null,9139,"27_15/11/2019 4:33:13 PM","2019-11-06","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","E/R - flow indicator for automatice air control unit for aft seal & S/T was found to be opaque.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Flow indicator glass cleaned up.","2019-12-31","","Completed","2019-11-30","No","No","No","Internal"]
[null,null,null,null,9140,"27_30/11/2019 1:49:15 PM","2019-11-25","Other","Ship Staff","Ship Staff Insp.","Vaccum condenser sea water pipe(flanged elbow) after the outlet valve leaking","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","New pipe fabricated (NB 500mmx 1200m Length) ,2 coats of epoxy applied and fitted in place.","2019-12-15","","Completed","2019-11-29","No","No","No","Internal"]
[null,null,null,null,9141,"27_30/11/2019 1:54:09 PM","2019-11-26","Other","Ship Staff","Ship Staff Insp.","Sea water inlet  pipe to cooler for Aft hyd.mooring system leaking from the weld seam.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Pipe welded at the weld seam and fitted back in place.Tried out-no leaks.","2019-12-23","","Completed","2019-11-30","No","No","No","Internal"]
[null,null,null,null,9142,"27_15/11/2019 4:28:22 PM","2019-11-06","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","E/R - bottom platform some of the securing screws for the platform plates ae missing","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","To secure all the platform plates with screws","2019-12-15","","Completed","2019-11-18","No","No","No","Internal"]
[null,null,null,null,9143,"27_16/11/2019 08:18:12","2019-11-06","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Lower Bearing Temperature for No.3 COP was bserved high during discharging compared to No.1 & No.2 COP","Cargo Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","New grease replaced and will observe temp rise during discharge.","2019-11-30","","Completed","2019-12-01","No","No","No","Internal"]
[null,null,null,null,9144,"27_16/11/2019 08:16:13","2019-11-06","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Upper Pump Bearing Temperature for COP 1 was observed high during Discharging compared to COP 2 & 3","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","Grease replaced and will observe temp.rise during discharge.","2019-11-30","","Completed","2019-12-01","No","No","No","Internal"]
[null,null,null,null,9145,"27_Fri Apr 12 2019 13:43:52 GMT+0000 (Coordinated Universal Time)","2019-12-01","Other","Ship Staff","Ship Staff Insp.","M/E Unit no.3 and 7 local exh.gas temp.gauge defective.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Temperature gauges renewed.","2019-12-20","","Completed","2019-12-03","No","No","No","Internal"]
[null,null,null,null,9146,"27_Wed Dec 04 2019 13:52:44 GMT+0000 (Coordinated Universal Time)","2019-12-01","Other","Ship Staff","Ship Staff Insp.","M/E RPSL Pump no.2 tripping on overload.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Pump and motor overhauled.Now it is operating satisfactory.","2019-12-20","","Completed","2019-12-04","No","No","No","Internal"]
[null,null,null,null,9147,"27_16/11/2019 10:36:49 AM","2019-11-06","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","The duty mess room bulkheads were dirty with oil/grease stain on bulkhead in some locations.","Accommodation","General Appearance","Human Error","","","","","Bulkheads cleaned","2019-12-31","","Completed","2019-12-06","No","No","No","Internal"]
[null,null,null,null,9148,"27_16/11/2019 07:15:25","2019-11-06","Critical Equipment,Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","3 Light shades in Engine Room were found broken or securing clamps Missing","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","Light shades renewed and Securing Clamps repaired","2019-11-30","","Completed","2019-12-06","No","No","No","Internal"]
[null,null,null,null,9149,"27_43779.6572569444","2019-09-13","Other","Ship Staff","Ship Staff Insp.","Diffusers for light fittings in engine room  damaged/cracked/broken at various locations post dd ","Critical Equip.,Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.25","Very High","","","Diffusers replaced as required.","2019-10-30","","Completed","2019-12-06","No","No","No","Internal"]
[null,null,null,null,9150,"27_Sun Nov 10 2019 15:49:57 GMT+0000 (Coordinated Universal Time)","2019-09-13","Other","Ship Staff","Ship Staff Insp.","Engine room alarm column light and sound non functional in various locations post dd","Cargo Mach.,Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.15","Low","","","E/R alarm columns made operational ","2019-10-30","DLOT190205","Completed","2019-12-07","No","No","No","Internal"]
[null,null,null,null,9151,"27_16/11/2019 06:33:47","2019-11-06","Critical Equipment,Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","No.1 Cargo Line Pressure Gauge not Working in CCR","Miscellaneous","Cargo / Ballast Systems","Equipment Related","","","","","Cargo line to the pressure transmitter found choked and same claered.Pr.transmitter calibrated and compared raed out with the gauge in CCR-all in ordeer.","2019-11-30","","Completed","2019-12-10","No","No","No","Internal"]
[null,null,null,null,9152,"27_15/11/2019 2:04:35 PM","2019-11-06","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","LSMGO line manifold marking missing. Some flange bolts are short in length. Drain pipe and vent pipe located on top has valve fitted but no blank.","Deck - Pipe / Fittings","MARPOL Related","Equipment Related","","","","","LSMGO Bunker line stenciled.Blank plugs installed \n\nand valve flange  small bolts replaced with longer ones.","2019-11-30","","Completed","2019-12-02","No","No","No","Internal"]
[null,null,null,null,9153,"27_Sat Oct 12 2019 20:16:46 GMT+0000 (Coordinated Universal Time)","2019-12-02","Other","Ship Staff","Ship Staff Insp.","A/Es fuel oil heater no.1 leaking from the end cover gasket","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Heater cleaned and end cover gasket renewed.","2019-12-28","","Completed","2019-12-06","No","No","No","Internal"]
[null,null,null,null,9154,"27_Sat Oct 12 2019 20:20:52 GMT+0000 (Coordinated Universal Time)","2019-12-03","","Ship Staff","Ship Staff Insp.","Aux.boiler no.2 main steam stop valve bonnet gasket passing.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Bonnet gasket renewed.","2019-12-30","","Completed","2019-12-08","No","No","No","Internal"]
[null,null,null,null,9155,"27_Sat Oct 12 2019 20:24:37 GMT+0000 (Coordinated Universal Time)","2019-12-03","Other","Ship Staff","Ship Staff Insp.","A/Es fuel oil heater no.2 leaking from the end cover gasket","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Heater cleaned and end cover gasket renewed.","2019-12-31","","Completed","2019-12-09","No","No","No","Internal"]
[null,null,null,null,9156,"27_Thu Dec 12 2019 07:56:06 GMT+0000 (Coordinated Universal Time)","2019-12-04","Other","Ship Staff","Ship Staff Insp.","Aux.Boiler's fuel oil pump no.2 mech seal leaking.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Pump seal renewed and electric motor o,hauled.","2019-12-31","","Completed","2019-12-11","No","No","No","Internal"]
[null,null,null,null,9157,"27_15/11/2019 1:43:34 PM","2019-11-06","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Slight vapour leak from 3C and 5C COT PV valve vacuum side","Deck - Pipe / Fittings,Hull & Tanks","MARPOL Related","Equipment Related","","","","","SEAT CLEANED AND ADJUSTED, NO MORE LEAKING","2019-11-30","","Completed","2019-11-25","No","No","No","Internal"]
[null,null,null,null,9158,"27_16/11/2019 10:24:09 AM","2019-11-06","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","CCR - No1 manifold pressure gauge not working","Cargo Mach.,Elect. Mach. & Equip.","Cargo / Ballast Systems","Equipment Related","","","","","NO 1 MANIFOLD PRESS GAUGE / TRANSMITER NEAR NO1 CARGO LINE AT MIDSHIP CALIBRATED, LINE BLOWN THROUGH, PRESSURE READING COMPAIRED WITH CCR GAUGE, IDENTICAL READING OBSERVED.","2019-12-31","`","Completed","2019-12-10","No","No","No","Internal"]
[null,null,null,null,9159,"27_16/11/2019 10:27:32 AM","2019-11-06","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","CCR - Continiuous alarm in the anemometer located in CCR. Once it is switched OFF, cannot be switched ON easily.","Elect. Mach. & Equip.","Cargo / Ballast Systems","Equipment Related","","","","","old anemometer unit showing ok now no more alarm, vessel received new anemometer on 23/11/2019 at galle. If old unit showing malfunction again we will renew.","2020-01-31","","Completed","2019-11-18","No","No","No","Internal"]
[null,null,null,null,9160,"27_16/11/2019 10:39:11 AM","2019-11-06","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Proper securing arrangement to be made for the weights in gymnasium.","Accommodation ,Miscellaneous","General Appearance","Equipment Related","","","","","All weights are properly secured in weight stag and weight stag is properly secured with the bulkhead","2019-12-31","","Completed","2019-11-19","No","No","No","Internal"]
[null,null,null,null,9161,"27_16/11/2019 10:34:34 AM","2019-11-06","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","The D-Link box located in the DT & CT locker room located opposite side of the CCR was kept loose.","Elect. Mach. & Equip.","Communication","Equipment Related","","","","","Box removed from the cabinet and secured in poop deck bosun store.","2020-01-31","","Completed","2019-11-22","No","No","No","Internal"]
[null,null,null,null,9162,"27_15/11/2019 1:57:47 PM","2019-11-06","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","STBD side hose handling crane's hydraulic hoses are not secured/bunched together","Deck - Machinery","General Appearance","Equipment Related","","","","","All secured/bunched together with cable tie","2019-11-30","","Completed","2019-11-27","No","No","No","Internal"]
[null,null,null,null,9163,"27_15/11/2019 2:13:59 PM","2019-11-06","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","STBD side bridge wing - manouevring console has debris located inside the covering","Navigation - Others","Navigation","Equipment Related","","","","","cleaned the console, all debris dust removed","2019-11-15","","Completed","2019-11-19","No","No","No","Internal"]
[null,null,null,null,9164,"27_15/11/2019 2:23:47 PM","2019-11-06","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","STBD side liferaft latest inspection date done on Sep 2019 label missing.","LSA / FFA","LSA / FFA Appliances","Human Error,Inappropriate Procedure","","","",""," labelled/marked, job done","2019-11-30","","Completed","2019-11-25","No","No","No","Internal"]
[null,null,null,null,9165,"27_16/11/2019 06:35:58","2019-11-06","Critical Equipment,Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Anemometer in CCR showing error ","Navigation - Others","Navigation","Equipment Related","","","","","Old anemometer now working fine with no alarm, recvd new set at galle","2019-11-30","","Completed","2019-11-18","No","No","No","Internal"]
[null,null,null,null,9166,"27_16/11/2019 06:39:17","2019-11-06","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","D-Link box in A Deck Duct not secured","Navigation - Others","Communication","Behaviour Based,Human Error","","","","","Box secured in poop deck bosun store","2019-11-30","","Completed","2019-11-22","No","No","No","Internal"]
[null,null,null,null,9167,"27_16/11/2019 06:42:20","2019-11-06","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","No proper securing arrangement for weights in Gymnasium ","Miscellaneous","MLC Related","Behaviour Based,Human Error","","","","","Fabrication of secured arrangement done, now secured","2019-11-30","","Completed","2019-11-19","No","No","No","Internal"]
[null,null,null,null,9168,"27_15/11/2019 2:26:07 PM","2019-11-06","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Some of SI lights for the lifebuoys had all the markings missing, including expiry date etc.","LSA / FFA","LSA / FFA Appliances","Equipment Related","","","","","Missing details posted","2019-11-30","","Completed","2019-11-25","No","No","No","Internal"]
[null,null,null,null,9169,"27_15/11/2019 2:43:15 PM","2019-11-06","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Observation tank for the slop tank steam coils - the glass view has been blanked.\n\nThe observation tank has to be covered in canvas.\n\nAlso one bolt for the retainer ring is missing.","Deck - Machinery,Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","","","","","Glass view blkank  reomved.\n\nTo be covered with canvas when not in use.\n\nOne missing  bolt fitted in place","2019-11-30","","Completed","2019-11-14","No","No","No","Internal"]
[null,null,null,null,9170,"27_15/11/2019 2:09:49 PM","2019-11-06","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Elecator escape/maintenance hatches on PORT side bridge wing has no markings","Miscellaneous","Emgcy. Systems","Inappropriate Procedure","","","","","stencilling done","2019-11-30","","Completed","2019-11-27","No","No","No","Internal"]
[null,null,null,null,9171,"27_15/11/2019 2:57:03 PM","2019-11-06","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Pumproom - slight oil leak from the glands of the stripping pump","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","Leakage arrested ","2019-11-30","","Completed","2019-11-28","No","No","No","Internal"]
[null,null,null,null,9172,"27_15/11/2019 4:21:45 PM","2019-11-06","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Steering gear room - Hyd oil tank for mooring - evidence of slight leak from the lvel indicator. Also the lower plunger valve was stuck in open position.","Deck - Mooring Machinery","Eng. / Strg. Comp.","Equipment Related","","","","","Leakage rectified by renewing the o-rings.","2019-12-15","","Completed","2019-12-16","No","No","No","Internal"]
[null,null,null,null,9173,"27_21/12/2019 1:57:12 PM","2019-12-21","Other","Ship Staff","Ship Staff Insp.","A/E 2 fuel oil inlet temp.sensor faulty.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Sensor cleaned and observed to be functioning satisfactory","2020-03-31","","Completed","2019-12-23","No","No","No","Internal"]
[null,null,null,null,9174,"27_25/12/2019 6:19:41 AM","2019-12-21","Other","Ship Staff","Ship Staff Insp.","AEs Fuel oil heater end cover gasket leaking","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Heaters removed from place,cleaned up and end cover gasket renewed.","2019-12-31","","Completed","2019-12-23","No","No","No","Internal"]
[null,null,null,null,9175,"27_25/12/2019 6:23:36 AM","2019-12-23","Other","Ship Staff","Ship Staff Insp.","IG scrubber sea water inlet valve from deck seal pump leaking.","Inert Gas","Eng. / Strg. Comp.","Equipment Related","","","","","Valve renewed with a spare one.","2019-12-31","","Completed","2019-12-24","No","No","No","Internal"]
[null,null,null,null,9176,"27_16/11/2019 07:11:24","2019-11-06","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Indications of leak from the seal of Low Expansion foam pump","Critical Equip.,LSA / FFA","LSA / FFA Appliances","Equipment Related","","","","","Currently no leaks observed.","2019-11-30","","Completed","2019-12-24","No","No","No","Internal"]
[null,null,null,null,9177,"27_15/11/2019 2:47:08 PM","2019-11-06","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Port side windlass - the wheel for the disk brake should be covered as same has been decommissioned","Deck - Machinery","Mooring","Equipment Related","","","","","AS THE BRAKE DRUM ROTATING WITH THE ROTATION OF GYPSY AND WINCH DRUM HENCE CAN NOT BE COVERED","2019-11-30","","Completed","2019-12-24","No","No","No","Internal"]
[null,null,null,null,9178,"27_Sun Nov 10 2019 16:17:26 GMT+0000 (Coordinated Universal Time)","2019-10-02","Other","Ship Staff","Ship Staff Insp.","No 1 Stbd Cargo tank temperature sensor is non functional ","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.37","High","","","Techincian attended the V/L at Singapore on 18th Nov.2019 and suggested to renew the junction box which V/L will install as the time permits.","2019-11-30","","Completed","2019-12-26","No","No","No","Internal"]
[null,null,null,null,9179,"27_15/11/2019 2:50:38 PM","2019-11-06","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Pumproom davit located outside pumproom entrance has all the gears exposed - cover is missing","Deck - Machinery","Emgcy. Systems","Equipment Related","","","","","Cover  fitted on exposed gears","2019-11-30","","Completed","2019-12-26","No","No","No","Internal"]
[null,null,null,null,9180,"27_15/11/2019 05:35:59","2019-11-06","Critical Equipment","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","Alrams Active on No.1 & No.2 UPS on Bridge","Critical Equip.,Elect. Mach. & Equip.","Emgcy. Systems","Equipment Related","","","",""," NO 1 UPS RENEWED BY SHORE TECHNICIAN AT SINGAPORE AND ALL FOUND TO BE IN ORDER.","2019-11-30","","Completed","2019-12-26","No","No","No","Internal"]
[null,null,null,null,9181,"27_16/11/2019 07:47:04","2019-11-06","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Main Engine Aft Scavanage air Cooler - Forward end was found leaking","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Defect deferred to DD and Refman made for the same","2019-11-30","","Completed","2019-12-26","No","No","No","Internal"]
[null,null,null,null,9182,"27_16/11/2019 8:36:16 AM","2019-11-01","Critical Equipment","Ship Staff","Ship Staff Insp.","Bridge UPS was not operational\t\t","Navigation - Others","Navigation","Equipment Related","","","",""," NO 1 UPS RENEWED BY SHORE TECHNICIAN AT SINGAPORE ON 18TH DEC 2019 AND ALL FOUND TO BE IN ORDE4R. OBSERVATION","2019-11-30","","Completed","2019-12-26","No","No","No","Internal"]
[null,null,null,null,9183,"27_16/11/2019 06:22:34","2019-11-06","Critical Equipment,Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Fire Line Pressure Gauge in CCR showing Erratic Reading","LSA / FFA","LSA / FFA Appliances","Equipment Related","","","","","Pressure transmitter needs renewal.Will raise RO for the same.","2019-11-30","","Completed","2019-12-26","No","No","No","Internal"]
[null,null,null,null,9184,"27_Sun Nov 10 2019 16:22:13 GMT+0000 (Coordinated Universal Time)","2019-10-10","Other","Ship Staff","Ship Staff Insp.","Draft gauges are non functional ","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.2","Medium","","","Technician expects to attend V/L at Zhoushan  about 28th Dec.2019","2019-11-30","DLOT 190219 ","Completed","2019-12-26","No","No","No","Internal"]
[null,null,null,null,9185,"27_16/11/2019 10:13:37 AM","2019-11-06","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","CCR - Stroke indicator for stripper pump is not showing the correct stroke value at times - same to be further investigated","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","To be investigated.","2019-12-31","","Completed","2019-12-26","No","No","No","Internal"]
[null,null,null,null,9186,"27_16/11/2019 10:10:13 AM","2019-11-06","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","CCR - Draught gauge not showing correct draughts","Miscellaneous","Navigation","Equipment Related","","","","","Shore technician expects to attend V/L at Zhoushan about 28th Dec.2019","2019-12-31","","Completed","2019-12-26","No","No","No","Internal"]
[null,null,null,null,9187,"27_16/11/2019 10:19:00 AM","2019-11-06","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","CCR - 2nd hydraulic pump does not cut-in automatically when the pressure in the system drops below the set value.","Deck - Machinery","Cargo / Ballast Systems","Equipment Related","","","","","Will raise RO in Jan'20","2020-01-31","","Completed","2019-12-26","No","No","No","Internal"]
[null,null,null,null,9188,"27_16/11/2019 10:15:58 AM","2019-11-06","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp."," - gas flow sensor for fixed gsa detection system was bypassed. Spares have been received - same to be fixed back in place","Cargo Mach.,Elect. Mach. & Equip.","Cargo / Ballast Systems","Equipment Related","","","","","2Nos.Mist catcher renewed.New Gas pump fitted in place,tried out and found to be turning hard.On further investigation ,motor winding found to be open ckted.Will land pump with the supplier at Singapore about 10th Jan 2020.","2019-12-31","","Completed","2019-12-26","No","No","No","Internal"]
[null,null,null,null,null,"27_2019-11-10 15:41:11.000","2019-09-13","Critical Equipment","Ship Staff","Ship Staff Insp.","Fire alarm showing fault ","LSA / FFA","LSA / FFA Appliances","Equipment Related",5.35,"Medium","Not Applicable","Not Applicable","Smoke sensor and manual call point needed for attendence. \r\nSmoke sensor and manual call point sensor renewed and found satisfactory.","2019-10-30","dlot190178 and dlot190210","Completed","2019-10-28","No",null,null,"Internal"]
[null,null,null,null,null,"27_2019-11-10 15:46:27.000","2019-09-13","Other","Ship Staff","Ship Staff Insp.","Diffusers for light fittings in engine room  damaged/cracked/broken at various locations post dd ","Critical Equip.,Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related",10.25,"Very High","Not Applicable","Not Applicable","Diffusers replaced as required","2019-10-30",null,"Completed","2019-12-06","No",null,null,"Internal"]
[null,null,null,null,null,"27_2019-11-10 15:49:57.999","2019-09-13","Other","Ship Staff","Ship Staff Insp.","Engine room alarm column light and sound non functional in various locations post dd","Cargo Mach.,Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related",10.15,"Low","Not Applicable","Not Applicable","Engine room alarm columns made operational ","2019-10-30","dlot190205","Completed","2019-12-07","No",null,null,"Internal"]
[null,null,null,null,null,"27_2019-11-10 15:53:50.000","2019-09-18","Other","Ship Staff","Ship Staff Insp.","A/E no 3 crank case getting pressurized ","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","A/E no.3 crankcase vent line newly fabricated to nominal dia 80A as per maker's recommendation","2019-12-31","dlot 190216","Completed","2019-11-17","No",null,null,"Internal"]
[null,null,null,null,null,"27_2019-11-10 15:58:11.999","2019-09-20","Other","Ship Staff","Ship Staff Insp.","LSMGO Main line manifold valve is not with gear operated ","Deck - Pipe / Fittings","Eng. / Strg. Comp.","Equipment Related",6.7,"High","Not Applicable","Not Applicable","LSMGO main line manifold fitted with gear operated valves","2019-12-30","dlot 190216","Completed","2019-11-25","No",null,null,"Internal"]
[null,null,null,null,null,"27_2019-11-10 16:13:17.000","2019-09-26","Other","Ship Staff","Ship Staff Insp.","Pumproom gas detection system sensor non functional ","Cargo Mach.","Cargo / Ballast Systems","Equipment Related",8.2100000000000009,"High","Not Applicable","Not Applicable","Pumproom Bottom STBD HC sensor renewed","2019-11-30","dlot 190008","Completed","2019-11-14","No",null,null,"Internal"]
[null,null,null,null,null,"27_2019-11-10 16:15:19.000","2019-10-02","Other","Ship Staff","Ship Staff Insp.","Anemometer in CCR is non functional ","Cargo Mach.","Cargo / Ballast Systems","Equipment Related",5.9,"Very High","Not Applicable","Not Applicable","Restored the windows in the system  - functioning satisfactorily","2019-10-30",null,"Completed","2019-11-05","No",null,null,"Internal"]
[null,null,null,null,null,"27_2019-11-10 16:17:26.999","2019-10-02","Other","Ship Staff","Ship Staff Insp.","No 1 Stbd Cargo tank temperature sensor is non functional ","Cargo Mach.","Cargo / Ballast Systems","Equipment Related",8.3699999999999992,"High","Not Applicable","Not Applicable","Technician attendance the V/L at Singapore on 18NOV2019 and suggested to renew the junction box which vessel will install as the time permits","2019-11-30",null,"Completed","2019-12-26","No",null,null,"Internal"]
[null,null,null,null,null,"27_2019-11-10 16:22:13.999","2019-10-10","Other","Ship Staff","Ship Staff Insp.","Draft gauges are non functional ","Cargo Mach.","Cargo / Ballast Systems","Equipment Related",8.1999999999999993,"Medium","Not Applicable","Not Applicable","Technician expects to attend vessel at Zhoushan about 28DEC2019","2019-11-30","DLOT 190219 ","Completed","2019-12-26","No",null,null,"Internal"]
[null,null,null,null,null,"27_2019-11-10 16:15:18.999","2019-10-02","Other","Ship Staff","Ship Staff Insp.","Anemometer in CCR is non functional ","Cargo Mach.","Cargo / Ballast Systems","Equipment Related",5.9,"Very High","Not Applicable","Not Applicable","Restored windows in the system - functioning satiisfactory","2019-10-30",null,"Completed","2019-11-05","No",null,null,"Internal"]
[null,null,null,null,null,"27_2019-11-10 16:20:15.000","2019-10-04","Defect","Ship Staff","Ship Staff Insp.","A/E no 3 smoke and heat detector is getting activated in heat mode while DG is in operation ","E/R - Aux. Mach.,LSA / FFA","Eng. / Strg. Comp.","Equipment Related",5.35,"Medium","Not Applicable","Not Applicable","Detectors to be repositioned to higher areas ","2019-11-30",null,"Completed","2019-10-17","No",null,null,"Internal"]
[null,null,null,null,null,"27_2019-11-10 16:25:11.999","2019-10-10","Other","Ship Staff","Ship Staff Insp.","Stbd Windlass brake assembly leaky due to scoring of rams ","Deck - Machinery,Deck - Mooring Machinery","Mooring","Equipment Related",9.14,"Medium","Not Applicable","Not Applicable","Shaft build up Belzona and smoothened. Seals replaced.","2019-10-30",null,"Completed","2019-11-01","No",null,null,"Internal"]
[null,null,null,null,null,"27_05/01/2020 4:23:43 PM","2020-01-01","Other","Ship Staff","Ship Staff Insp.","LT Cooler no.2 sea water inlet valve leaking from the valve body.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related",null,null,"Not Applicable","Not Applicable","Valave replaced with the new one.","2020-01-31",null,"Completed","2020-01-01","No",null,null,"Internal"]
[null,null,null,null,null,"27_07/01/2020 4:44:48 PM","2020-01-04","Observation","Ship Staff","Ship Staff Insp.","Hot water calorifier electric motor making abnormal noise.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related",null,null,"Not Applicable","Not Applicable","Motor dismantled,inspected and bearings renewed.","2020-01-30",null,"Completed","2020-01-04","No",null,null,"Internal"]
[null,null,null,null,null,"27_23/12/2019 6:14:06 PM","2019-12-21","Other","Ship Staff","Ship Staff Insp.","Scruuber overboard pipe observed to be partly clogged.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related",null,null,"Not Applicable","Not Applicable","Overboard valve closed and oboard pipe drained off water.Removed NRV from place which was found to be fully clogged with polyeuthrene coating.Scrubber pump tried out -satisfactory.","2020-01-31",null,"Completed","2020-01-06","No",null,null,"Internal"]
[null,null,null,null,null,"27_16/11/2019 10:07:33 AM","2019-11-06","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Fire line pressure in CCR doesn't show the correct reading. Always showing 2 bar.","LSA / FFA","LSA / FFA Appliances","Equipment Related",null,null,"Not Applicable","Not Applicable","Renewed pressure transmitter.Gauge in the CCR shows correct read out.","2019-11-30",null,"Completed","2020-01-06","No",null,null,"Internal"]
[null,null,null,null,null,"27_16/11/2019 06:31:43","2019-11-06","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","SAAB Buzzer in CCR not audible","Miscellaneous","Cargo / Ballast Systems","Equipment Related",null,null,"Not Applicable","Not Applicable","Will modify the ckt","2019-11-30",null,"Completed","2020-01-06","No",null,null,"Internal"]
[null,null,null,null,null,"27_14/01/2020 9:55:58 AM","2020-01-04","Other","Ship Staff","Ship Staff Insp.","Main engine jacket water pre-heating pump motor making abnormal noise","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related",null,null,"Not Applicable","Not Applicable","Motor o'hauled with new bearings.","2020-04-05",null,"Completed","2020-01-05","No",null,null,"Internal"]

{"sheet":"Calc","index":2,"n_rows":28,"n_cols":12,"rows_kept":28,"cut":false,"hidden":true,"merged":[]}
["Def_type","Def_cause","Equipments","VIQrefno","Observer_code"]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,"Dim itemSele As Long"]
[null,null,null,null,null,null,null,null,null,null,null,"   dim startRow as integer"]
[null,null,null,null,null,null,null,null,null,null,null,"   startRow=1"]
[null,null,null,null,null,null,null,null,null,null,null,"        For itemSele = 0 To ListBox1.ListCount - 1"]
[null,null,null,null,null,null,null,null,null,null,null,"        If ListBox1.Selected(itemSele) = True Then"]
[null,null,null,null,null,null,null,null,null,null,null,"        Worksheets(\"WorksheetName\").Range(\"A\" & startRow).Value = ListBox1.List(itemSele)"]
[null,null,null,null,null,null,null,null,null,null,null,"        startRow = startRow + 1"]
[null,null,null,null,null,null,null,null,null,null,null,"        End If"]
[null,null,null,null,null,null,null,null,null,null,null,"        Next"]
[null,null,null,null,null,null,null,null,null,null,null,"Dim LastRowA As String"]
[null,null,null,null,null,null,null,null,null,null,null,"        Dim itemSele As Long"]
[null,null,null,null,null,null,null,null,null,null,null,"       Dim startRow as integer"]
[null,null,null,null,null,null,null,null,null,null,null,"        LastRowA = ActiveSheet.Cells(Rows.count, \"A\").End(xlUp).row"]
[null,null,null,null,null,null,null,null,null,null,null,"        startQue = 0"]
[null,null,null,null,null,null,null,null,null,null,null,"        For itemSele = 0 To ListBox1.ListCount - 1"]
[null,null,null,null,null,null,null,null,null,null,null,"        For startRow = 1 To LastRowA"]
[null,null,null,null,null,null,null,null,null,null,null,"        If Worksheets(\"WorksheetName\").Range(\"A\" & startRow).Value = ListBox1.List(itemSele) Then"]
[null,null,null,null,null,null,null,null,null,null,null,"        ListBox1.Selected(itemSele) = True"]
[null,null,null,null,null,null,null,null,null,null,null,"        Exit For"]
[null,null,null,null,null,null,null,null,null,null,null,"        End If"]
[null,null,null,null,null,null,null,null,null,null,null,"        Next j"]
[null,null,null,null,null,null,null,null,null,null,null,"        Next"]
[null,null,null,null,null,null,null,null,null,null,null,"        End If"]

{"sheet":"Areaofobs","index":3,"n_rows":17,"n_cols":2,"rows_kept":17,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Cargo / Ballast Systems",11]
["Cert. & Docu.",2]
["Communication",6]
["Crew Management",3]
["Emgcy. Systems",13]
["Eng. / Strg. Comp.",14]
["General Appearance",15]
["Ice Opns.",17]
["ISM Related",7]
["ISPS Related",10]
["LSA / FFA Appliances",8]
["MARPOL Related",9]
["MLC Related",4]
["Mooring",12]
["Navigation",5]
["Structural Condn. / WT integrity ",16]

{"sheet":"Vessel_type","index":4,"n_rows":1,"n_cols":2,"rows_kept":1,"cut":false,"hidden":true,"merged":[]}
["Vessel_type","ID"]

{"sheet":"Deficiency_type","index":5,"n_rows":8,"n_cols":3,"rows_kept":8,"cut":false,"hidden":true,"merged":[]}
["TITLE","Type of deficiency_description","ID"]
["Breakdown",null,6]
["Critical Equipment",null,4]
["Defect",null,1]
["Guarantee Claim",null,8]
["Non Conformity",null,2]
["Observation",null,3]
["Other",null,7]

{"sheet":"VIQrefno","index":6,"n_rows":427,"n_cols":3,"rows_kept":427,"cut":false,"hidden":true,"merged":[]}
["VIQ_ref_no","Risk Value of observation","ID"]
["1.1","Low",8243]
["1.10","Low",8252]
["1.11","Low",8253]
["1.12","Low",8254]
["1.13","Low",8255]
["1.14","Low",8256]
["1.15","Low",8257]
["1.16","Low",8259]
["1.17","Low",8260]
["1.18","Low",8261]
["1.19","Low",8262]
["1.2","Low",8244]
["1.20","Low",8263]
["1.21","Low",8265]
["1.22","Low",8266]
["1.23","Low",8267]
["1.24","Low",8268]
["1.25","Low",8269]
["1.26","Low",8270]
["1.3","Low",8245]
["1.4","Low",8246]
["1.5","Low",8247]
["1.6","Low",8248]
["1.7","Low",8249]
["1.8","Low",8250]
["1.9","Low",8251]
["1.99","High",11258]
["10.1","Medium",8461]
["10.10","High",8470]
["10.11","Medium",8471]
["10.12","Very High",8472]
["10.13","Very High",8473]
["10.14","Medium",8474]
["10.15","Low",8475]
["10.16","Very High",8476]
["10.17","Very High",8477]
["10.18","High",8478]
["10.19","Very High",8479]
["10.2","Low",8462]
["10.20","High",8480]
["10.21","Medium",8481]
["10.22","Low",8482]
["10.23","Medium",8483]
["10.24","Low",8484]
["10.25","Very High",8485]
["10.26","High",8486]
["10.27","Medium",8487]
["10.28","Low",8488]
["10.29","Medium",8489]
["10.3","Medium",8463]
["10.30","High",8490]
["10.31","Very High",8491]
["10.32","Very High",8492]
["10.33","High",8493]
["10.34","High",8494]
["10.35","Very High",8495]
["10.36","Very High",8496]
["10.37","Medium",8497]
["10.38","Medium",8498]
["10.39","High",8499]
["10.4","High",8464]
["10.40","Medium",8500]
["10.41","Medium",8501]
["10.42","Medium",8502]
["10.43","Medium",8503]
["10.44","Medium",8504]
["10.45","Very High",8505]
["10.46","High",8506]
["10.47","Medium",8507]
["10.48","High",8508]
["10.49","Medium",8509]
["10.5","Low",8465]
["10.50","High",8510]
["10.51","Low",8511]
["10.52","Medium",8512]
["10.53","Medium",8513]
["10.54","High",8514]
["10.55","Low",8515]
["10.6","Very High",8466]
["10.7","Medium",8467]
["10.8","Medium",8468]
["10.9","Medium",8469]
["10.99","High",8516]
["11.1","High",8420]
["11.10","Medium",8429]
["11.11","Very High",8430]
["11.12","Low",8431]
["11.13","Low",8432]
["11.14","Medium",8433]
["11.15","Low",8434]
["11.16","Low",8435]
["11.17","Low",8436]
["11.2","Medium",8421]
["11.3","Medium",8422]
["11.4","Very High",8423]
["11.5","Medium",8424]
["11.6","Medium",8425]
["11.7","High",8426]
["11.8","Low",8427]
["11.9","Low",8428]
["11.99","High",8437]
["12.1","High",8438]
["12.10","High",8448]
["12.11","High",8449]
["12.12","High",8450]
["12.13","High",8451]
["12.14","High",8452]
["12.15","High",8453]
["12.16","High",8454]
["12.17","High",8455]
["12.18","High",8456]
["12.19","High",8457]
["12.2","High",8439]
["12.20","High",8458]
["12.21","High",8459]
["12.3","High",8441]
["12.4","High",8442]
["12.5","High",8443]
["12.6","High",8444]
["12.7","High",8445]
["12.8","High",8446]
["12.9","High",8447]
["12.99","High",8460]
["2.1","Very High",8296]
["2.1.9","Very High",11259]
["2.10","Medium",8304]
["2.11","Medium",8305]
["2.12","Low",8306]
["2.13","Low",8307]
["2.14","Low",8308]
["2.15","Low",8309]
["2.16","Medium",8310]
["2.2","Medium",8297]
["2.3","High",8295]
["2.4","Medium",8298]
["2.5","Medium",8299]
["2.6","Low",8300]
["2.7","High",8301]
["2.8","High",8302]
["2.9","Medium",8303]
["2.99","High",8311]
["3.1","High",8312]
["3.2","Very High",8313]
["3.3","High",8314]
["3.4","Low",8294]
["3.5","Medium",8315]
["3.6","High",8316]
["3.7","Very High",8317]
["3.8","Very High",8318]
["3.99","High",8319]
["4.1","High",8320]
["4.10","High",8329]
["4.11","Medium",8330]
["4.12","Very High",8331]
["4.13","Very High",8332]
["4.14","Very High",8333]
["4.15","Very High",8334]
["4.16","Very High",8335]
["4.17","Very High",8336]
["4.18","Very High",8337]
["4.19","Low",8338]
["4.2","Medium",8321]
["4.20","Very High",8339]
["4.21","High",8340]
["4.22","Low",8341]
["4.23","High",8342]
["4.24","High",8343]
["4.25","Low",8344]
["4.26","Low",8345]
["4.27","High",8346]
["4.3","Medium",8322]
["4.4","High",8323]
["4.5","Very High",8324]
["4.6","Medium",8325]
["4.7","High",8326]
["4.8","Medium",8327]
["4.9","Medium",8328]
["4.99","High",8347]
["5.1","Very High",8517]
["5.10","High",8526]
["5.11","Low",8527]
["5.12","Medium",8528]
["5.13","High",8529]
["5.14","Very High",8530]
["5.15","Medium",8531]
["5.16","Very High",8532]
["5.17","Very High",8533]
["5.18","High",8534]
["5.19","Medium",8535]
["5.2","Very High",8518]
["5.20","Medium",8536]
["5.21","Medium",8537]
["5.22","High",8539]
["5.23","Very High",8540]
["5.24","Very High",8541]
["5.25","Medium",8542]
["5.26","Medium",8543]
["5.27","Medium",8544]
["5.28","Very High",8545]
["5.29","High",8546]
["5.3","Low",8519]
["5.30","High",8547]
["5.31","High",8548]
["5.32","High",8549]
["5.33","High",8550]
["5.34","Low",8551]
["5.35","Medium",8552]
["5.36","Low",8553]
["5.37","Low",8554]
["5.38","High",8555]
["5.39","Very High",8556]
["5.4","High",8520]
["5.40","Very High",8557]
["5.41","Very High",8558]
["5.42","Medium",8559]
["5.43","High",8560]
["5.44","High",8561]
["5.45","Medium",8564]
["5.46","Medium",8565]
["5.47","Medium",8566]
["5.48","Medium",8567]
["5.5","Low",8521]
["5.6","Low",8522]
["5.7","Medium",8523]
["5.8","Medium",8524]
["5.9","Very High",8525]
["5.99","High",8568]
["6.1","Medium",8348]
["6.10","Low",8357]
["6.11","High",8358]
["6.12","Medium",8359]
["6.13","Low",8360]
["6.14","High",8361]
["6.15","High",8362]
["6.16","Very High",8363]
["6.17","Very High",8364]
["6.18","Medium",8365]
["6.19","Low",8366]
["6.2","High",8349]
["6.20","Medium",8367]
["6.21","High",8368]
["6.22","Medium",8369]
["6.3","Low",8350]
["6.4","High",8351]
["6.5","Medium",8352]
["6.6","Medium",8353]
["6.7","High",8354]
["6.8","High",8355]
["6.9","Low",8356]
["6.99","High",8370]
["7.1","High",8371]
["7.10","High",8380]
["7.11","High",8381]
["7.12","High",8382]
["7.13","Medium",8383]
["7.14","Medium",8384]
["7.15","High",8385]
["7.16","High",8386]
["7.17","High",8387]
["7.2","High",8372]
["7.3","Low",8373]
["7.4","Low",8374]
["7.5","Low",8375]
["7.6","Medium",8376]
["7.7","Low",8377]
["7.8","High",8378]
["7.9","High",8379]
["7.99","High",8388]
["8.1","Very High",8569]
["8.10","Very High",8578]
["8.100","Low",11227]
["8.101","Medium",11228]
["8.102","Low",11229]
["8.103","Low",11230]
["8.104","Low",11231]
["8.105","Medium",11232]
["8.106","Medium",11233]
["8.107","Low",11234]
["8.108","High",11235]
["8.109","Very High",11236]
["8.11","Medium",8579]
["8.110","High",11237]
["8.111","Medium",11238]
["8.112","High",11239]
["8.113","Medium",11240]
["8.114","Low",11241]
["8.115","High",11242]
["8.116","Medium",11243]
["8.117","Medium",11244]
["8.118","Medium",11245]
["8.119","High",11246]
["8.12","Medium",8580]
["8.120","High",11247]
["8.121","Medium",11248]
["8.122","High",11249]
["8.123","High",11250]
["8.124","Low",11251]
["8.125","High",11252]
["8.126","Medium",11253]
["8.127","Medium",11254]
["8.13","Medium",8581]
["8.14","Very High",8582]
["8.15","High",8583]
["8.16","Very High",8584]
["8.17","Low",8585]
["8.18","High",8586]
["8.19","High",8587]
["8.199","High",11255]
["8.2","Medium",8570]
["8.20","Medium",8588]
["8.21","High",8589]
["8.22","Very High",8590]
["8.23","Medium",8591]
["8.24","Medium",8592]
["8.25","Very High",8593]
["8.26","High",8594]
["8.27","Medium",8595]
["8.28","Medium",8596]
["8.29","High",8598]
["8.3","Very High",8571]
["8.30","High",8599]
["8.31","High",8600]
["8.32","Low",8601]
["8.33","Medium",8602]
["8.34","High",8603]
["8.35","Medium",8604]
["8.36","Medium",8605]
["8.37","High",8607]
["8.38","Medium",8608]
["8.39","Medium",8609]
["8.4","Medium",8572]
["8.40","High",8610]
["8.41","Medium",8611]
["8.42","Medium",8612]
["8.43","Very High",8613]
["8.44","High",8615]
["8.45","High",8616]
["8.46","Very High",8617]
["8.47","Very High",8618]
["8.48","Medium",8619]
["8.49","High",8620]
["8.5","Very High",8573]
["8.50","Medium",8621]
["8.51","Low",8622]
["8.52","Low",8623]
["8.53","Low",8624]
["8.54","High",8625]
["8.55","Low",11182]
["8.56","Medium",11183]
["8.57","Medium",11184]
["8.58","High",11185]
["8.59","High",11186]
["8.6","Medium",8574]
["8.60","High",11187]
["8.61","Medium",11188]
["8.62","Very High",11189]
["8.63","High",11190]
["8.64","Medium",11191]
["8.65","Low",11192]
["8.66","High",11193]
["8.67","High",11194]
["8.68","High",11195]
["8.69","Medium",11196]
["8.7","High",8575]
["8.70","Medium",11197]
["8.71","Very High",11198]
["8.72","Medium",11199]
["8.73","Medium",11200]
["8.74","High",11201]
["8.75","Medium",11202]
["8.76","Medium",11203]
["8.77","Medium",11204]
["8.78","Medium",11205]
["8.79","Medium",11206]
["8.8","Medium",8576]
["8.80","Medium",11207]
["8.81","Low",11208]
["8.82","Medium",11209]
["8.83","Low",11210]
["8.84","Low",11211]
["8.85","Medium",11212]
["8.86","Medium",11213]
["8.87","Medium",11214]
["8.88","Low",11215]
["8.89","High",11216]
["8.9","High",8577]
["8.90","High",11217]
["8.91","High",11218]
["8.92","Medium",11219]
["8.93","Low",11220]
["8.94","Low",11221]
["8.95","Medium",11222]
["8.96","Medium",11223]
["8.97","Low",11224]
["8.98","High",11225]
["8.99","Medium",11226]
["9.1","Low",8390]
["9.10","Medium",8399]
["9.11","Medium",8400]
["9.12","Medium",8401]
["9.13","Low",8402]
["9.14","Medium",8403]
["9.15","Medium",8404]
["9.16","High",8405]
["9.17","High",8406]
["9.18","Low",8407]
["9.19","Low",8408]
["9.2","Very High",8391]
["9.20","Medium",8409]
["9.21","Medium",8410]
["9.22","Low",8411]
["9.23","Low",8412]
["9.24","Medium",8413]
["9.25","Low",8414]
["9.26","Low",8415]
["9.27","Low",8416]
["9.28","Medium",8417]
["9.29","Low",8418]
["9.3","Very High",8392]
["9.4","High",8393]
["9.5","High",8394]
["9.6","Low",8395]
["9.7","Medium",8396]
["9.8","Medium",8397]
["9.9","Medium",8398]
["9.99","High",8419]

{"sheet":"Equipment_list","index":7,"n_rows":27,"n_cols":3,"rows_kept":27,"cut":false,"hidden":true,"merged":[]}
["TITLE","Equipment_list_description","ID"]
["Accommodation ",null,12]
["Cargo Mach.",null,13]
["Critical Equip.",null,16]
["Deck - Machinery",null,18]
["Deck - Mooring Machinery",null,15]
["Deck - Pipe / Fittings",null,20]
["Documentation",null,21]
["E/R - Air Comp.",null,8]
["E/R - Aux. Engine",null,4]
["E/R - Aux. Mach.",null,7]
["E/R - Boiler",null,5]
["E/R - Main Engine",null,3]
["E/R - Pipes/ valves & fittings",null,9]
["E/R - Purifier",null,6]
["Elect. Mach. & Equip.",null,10]
["Hull & Tanks",null,19]
["Inert Gas",null,14]
["LSA / FFA",null,17]
["Miscellaneous",null,22]
["Navigation - DGPS / EPFS / AIS",null,28]
["Navigation - ECDIS",null,25]
["Navigation - Echo Sounder / Speed Log",null,26]
["Navigation - GMDSS & Communication",null,23]
["Navigation - Others",null,11]
["Navigation - RADAR",null,24]
["Navigation - VDR / BNWAS",null,30]

{"sheet":"PSC_MOU","index":8,"n_rows":11,"n_cols":3,"rows_kept":11,"cut":false,"hidden":true,"merged":[]}
["TITLE","PSC_MOU_description","ID"]
["Asia and the Pacific",null,2]
["Caribbean",null,4]
["Europe and the North Atlantic",null,1]
["Latin America",null,3]
["The Black Sea region",null,6]
["The Indian Ocean",null,8]
["The Mediterranean",null,7]
["The Riyadh MoU",null,9]
["USCG",null,10]
["West and Central Africa",null,5]

{"sheet":"Inspection_type","index":9,"n_rows":11,"n_cols":2,"rows_kept":11,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Bunkering Audit",14]
["Engineering Audit",16]
["ISM Audit",2]
["ISPS Audit",3]
["IT Audit",10]
["MLC Audit",1]
["Mooring Audit",9]
["Nav Audit / Verification",8]
["Ship Staff Insp.",15]
["Suptd. Insp.",13]

{"sheet":"Deficiency_Cause","index":10,"n_rows":8,"n_cols":3,"rows_kept":8,"cut":false,"hidden":true,"merged":[]}
["TITLE","Deficiency_Cause_description","ID"]
["Behaviour Based",null,1]
["Equipment Related",null,4]
["External Factors",null,5]
["Human Error",null,7]
["Inappropriate Procedure",null,8]
["Industry Issue",null,6]
["Knowledge Based",null,3]

{"sheet":"Observer_code","index":11,"n_rows":3,"n_cols":3,"rows_kept":3,"cut":false,"hidden":true,"merged":[]}
["TITLE","Observer_code_description","ID"]
["Owner / Marine / Tech. Suptd.",null,3]
["Ship Staff",null,2]

{"sheet":"Status_code","index":12,"n_rows":6,"n_cols":3,"rows_kept":6,"cut":false,"hidden":true,"merged":[]}
["TITLE","Status_code_description","ID"]
["Completed",null,6]
["Deferred to D D",null,5]
["In progress",null,3]
["Not Started",null,2]
["Waiting spare",null,4]

{"sheet":"PSC_ref_no","index":13,"n_rows":19,"n_cols":2,"rows_kept":19,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Alarms",9]
["Cargo operations including equipment",7]
["Certificates & Documentation",2]
["Dangerous Goods",13]
["Emergency Systems",5]
["Fire safety",8]
["ISM",16]
["ISPS",17]
["Life saving appliances",12]
["MLC, 2006",18]
["Other",19]
["Pollution Prevention",15]
["Propulsion and auxiliary machinery",14]
["Radio communication",6]
["Safety of Navigation",11]
["Structural condition",3]
["Water/Weathertight condition",4]
["Working and Living Conditions",10]

{"sheet":"Risk_value_of_obs","index":14,"n_rows":1,"n_cols":2,"rows_kept":1,"cut":false,"hidden":true,"merged":[]}
["Risk Value of observation","ID"]

{"sheet":"Year","index":15,"n_rows":18,"n_cols":1,"rows_kept":18,"cut":false,"hidden":true,"merged":[]}
["Year"]
[2014]
[2015]
[2016]
[2017]
[2018]
[2019]
[2020]
[2021]
[2022]
[2023]
[2024]
[2025]
[2026]
[2027]
[2028]
[2029]
[2030]

{"sheet":"Month","index":16,"n_rows":13,"n_cols":1,"rows_kept":13,"cut":false,"hidden":true,"merged":[]}
["Month"]
["Jan"]
["Feb"]
["Mar"]
["Apr"]
["May"]
["Jun"]
["Jul"]
["Aug"]
["Sep"]
["Oct"]
["Nov"]
["Dec"]

{"sheet":"Date_","index":17,"n_rows":32,"n_cols":1,"rows_kept":32,"cut":false,"hidden":true,"merged":[]}
["Date"]
["01"]
["02"]
["03"]
["04"]
["05"]
["06"]
["07"]
["08"]
["09"]
[10]
[11]
[12]
[13]
[14]
[15]
[16]
[17]
[18]
[19]
[20]
[21]
[22]
[23]
[24]
[25]
[26]
[27]
[28]
[29]
[30]
[31]

{"sheet":"Sheet1","index":18,"n_rows":24,"n_cols":6,"rows_kept":24,"cut":false,"hidden":true,"merged":[]}
[]
[null,"ID","E",null,"Date Recorded",1]
[null,"UNIQUE ID","F",null,"Type of Deficiency",2]
[1,"Date Recorded","G",null,"Observer code",3]
["ignore","Vessel Type","H",null,"Type of Inspection",4]
[null,"Internal / External","I",null,"Description of Deficiency",5]
[null,"Drydock","J",null,"Equipment Categories",6]
[null,"Information Sharing","K",null,"Area of Observation",7]
[null,"Critical_item","L",null,"Deficiency Cause",8]
[null,"Deficiency Type","M",null,"VIQ Ref Number",9]
[null,"Deficiency Cause","N",null,"Risk Value of Obs",10]
[null,"Inspection Type","O",null,"PSC Ref Number",11]
[null,"Equipments","P",null,"PSC MOU ID",12]
[null,"VIQ Reference Number","Q",null,"Action Taken or Required",13]
[null,"Risk Value of the observation","R",null,"Target Date",14]
[null,"PSC Reference Number","S",null,"PO Ref No.",15]
[null,"PSC MOU","T",null,"Status Code",16]
[null,"Observer Code","U",null,"Date Completed",17]
[null,"Target Date","V",null,"Drydock",18]
[null,"Status Code","W",null,"Info Sharing",19]
[null,"Description of Deficiency","X",null,"Critical Item Flag",20]
[null,"Action taken / required","Y",null,"Audit Type",21]
[null,"PO ref no","Z"]
[null,"Date completed","AA"]

{"sheet":"Ship_information","index":19,"n_rows":2,"n_cols":3,"rows_kept":2,"cut":false,"hidden":true,"merged":[]}
["Ship_ID","Ship_Name","FILE_NAME"]
["27","DHT LOTUS (26-12-2019)","27_1577776246406.xlsm"]

{"sheet":"External_Deficiency_type","index":20,"n_rows":5,"n_cols":3,"rows_kept":5,"cut":false,"hidden":true,"merged":[]}
["TITLE","Type of deficiency_description","ID"]
["Condn of Class / Memo",null,5]
["Defect",null,1]
["Non Conformity",null,2]
["Observation",null,3]

{"sheet":"External_Inspection_type","index":21,"n_rows":10,"n_cols":2,"rows_kept":10,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Flag State Insp.",5]
["ISM Audit",2]
["ISPS Audit",3]
["MLC Audit",1]
["Nav Audit / Verification",8]
["OM Insp. (Eg. SIRE / CDI etc.)",6]
["Others (Eg. Insurance etc.)",12]
["PSC Inspection",4]
["Terminal Insp.",11]

{"sheet":"External_Observer_code","index":22,"n_rows":7,"n_cols":3,"rows_kept":7,"cut":false,"hidden":true,"merged":[]}
["TITLE","Observer_code_description","ID"]
["Class Surveyor",null,4]
["FSC Inspector",null,5]
["Others (Eg. Insurance etc.)",null,9]
["PSC Insp.",null,6]
["SIRE / CDI Insp.",null,8]
["Terminal Insp.",null,7]

{"sheet":"Sheet Version","index":23,"n_rows":2,"n_cols":2,"rows_kept":2,"cut":false,"hidden":true,"merged":[]}
["Version","Title"]
["2.0","Version 2.0"]