{"text_format":"1","workbook":"xlsx","n_sheets":24,"sheets":["Mainsheet","Completed","Calc","Areaofobs","Vessel_type","Deficiency_type","VIQrefno","Equipment_list","PSC_MOU","Inspection_type","Deficiency_Cause","Observer_code","Status_code","PSC_ref_no","Risk_value_of_obs","Year","Month","Date_","Sheet1","Ship_information","External_Deficiency_type","External_Inspection_type","External_Observer_code","Sheet Version"],"not_rendered":{"charts":0,"images":5,"macros":1,"external_links":0,"defined_names":12,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Mainsheet","index":0,"n_rows":43,"n_cols":28,"rows_kept":43,"cut":false,"hidden":false,"merged":[[10,8,10,9],[10,12,10,13],[12,6,12,27],[8,6,8,27]]}
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,"Defect - Damage Monitoring Sheet"]
[]
[null,null,null,null,null,null,null,"Date of Report","31-Dec-2019",null,null,"Ship Name","ATHERINA (26-12-2019)"]
[]
[null,null,null,null,null,null,"VERSION : 2.0"]
[]
[]
[]
[null,null,null,null,"ID","UNIQUE ID","Date Recorded","Type of Deficiency","Observer code","Type of Inspection","Description of Deficiency","Equipment Categories","Area of Observation","Deficiency Cause","VIQ Ref Number","Risk Value of Obs","PSC Ref Number","PSC MOU ID","Action Taken or Required","Target Date","PO Ref No.","Status Code","Date Completed","Drydock","Info Sharing","Critical Item","Audit Type","Superintendent Remarks"]
[null,null,null,null,2092,"83_16/10/2019 6:15:25 PM","2019-03-25","Defect","Ship Staff","Ship Staff Insp.","Composite boiler back firing occasionally, furnace space and smoke tubes water washed with high pressure as we saw lot of unburnt HFO in furnace and tubes. Air and fuel to adjust as steam pressure not coping up.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Kangrim service engineer attended the vessel at Singapore on 22nd April'19 and suggested that the tubes require chemical cleaning .This is reason for blowback due to high back pressure.","2019-12-30",null,"Not Started",null,"No","No","No","Internal"]
[null,null,null,null,2093,"83_16/10/2019 6:16:39 PM","2019-04-05","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Servo pump pressure drops very fast after stopping Main engine. Need to investigate the reason and repair.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Under investigation. No issues with the pressures when the Engine is running.","2019-12-30",null,"In progress",null,"No","No","No","Internal"]
[null,null,null,null,2094,"83_16/10/2019 6:18:27 PM","2019-04-10","Defect","Ship Staff","Ship Staff Insp.","ME Exhaust valve VCU rail valve timing reaching 1.5 ms . Will require replacement in due course.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","ME Performance taken and as of now rail valves timings are below 1.5 ms. RO for spares raised.","2019-09-30","ATHE190107, Item no-4","Waiting spare",null,"No","No","No","Internal"]
[null,null,null,null,2095,"83_16/10/2019 6:24:01 PM","2019-04-01","Defect","Ship Staff","Ship Staff Insp.","Deck seal flow sensor bypassed.","Inert Gas","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Flow switch to replaced but Flow relay in main panel found defective, Requisition ATHE190159 Raised.","2019-11-15","ATHE190159","Waiting spare",null,"No","No","No","Internal"]
[null,null,null,null,2100,"83_16/10/2019 6:31:38 PM","2019-06-02","Defect","Ship Staff","Ship Staff Insp.","M/E FO Viscotherm function erratic.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Suspect problem with the viscotherm sensor connected with the DP transmitter .","2019-11-15","ATHE190075\t","Waiting spare",null,"No","No","No","Internal"]
[null,null,null,null,2103,"83_17/10/2019 6:06:09 PM","2019-06-05","Defect","Ship Staff","Ship Staff Insp.","SALWICO Fixed gas detection system display screen in CCR showing erratic numbers & alphabets.","Miscellaneous","General Appearance","Equipment Related",8.4600000000000009,"Very High","Not Applicable","Not Applicable","PO raised, Spares will be supplied from Owner Side.","2019-09-30"," ATHE190078\t ","Waiting spare",null,"No","No","No","Internal"]
[null,null,null,null,2106,"83_17/10/2019 6:10:36 PM","2019-07-01","Defect","Ship Staff","Ship Staff Insp.","All Centre cargo tanks reading in K Guage tank radar system remote display in CCR not showing correct readings & some times gets frozen.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related",8.1199999999999992,"Medium","Not Applicable","Not Applicable","Technician need to attend and recaliberate.","2019-11-15"," \t ","Not Started",null,"No","No","No","Internal"]
[null,null,null,null,2108,"83_17/10/2019 6:13:50 PM","2019-08-06","Defect","Ship Staff","Ship Staff Insp.","Section of IG to Ballast line near Pumproom entrance found wasted & holed.\t","Inert Gas","General Appearance","Equipment Related",11.4,"Very High","Not Applicable","Not Applicable","Temporary repairs carried out - 08/08/19.\t","2019-10-30"," ","Deferred to D D",null,"No","No","No","Internal"]
[null,null,null,null,2109,"83_17/10/2019 6:15:17 PM","2019-08-20","Defect","Ship Staff","Ship Staff Insp.","New Oxygen analyzer reading of oxygen percentage is not steady causing IG deck and atmosphere valves to malfunction , Touch panel on same is defective.","Inert Gas","Eng. / Strg. Comp.","Equipment Related",8.25,"Very High","Not Applicable","Not Applicable","Need advice from maker to rectify fault, Kamlesh Solanki is looking in to matter.","2019-11-15"," \t","In progress",null,"No","No","No","Internal"]
[null,null,null,null,2111,"83_17/10/2019 6:18:49 PM","2019-08-17","Defect","Ship Staff","Ship Staff Insp.","Air Ejector use for vacuum condenser found crack on end plate .","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Pressure test carried out from fresh water side to check any tube leaking or sea water is mixing with fresh water. Pressure is holding during pressure test. Eventually need to repair .\t","2020-08-22"," ","Deferred to D D",null,"No","No","No","Internal"]
[null,null,null,null,2119,"83_17/10/2019 6:30:27 PM","2019-10-10","Defect","Ship Staff","Ship Staff Insp.","HFO purifer No-2 Bowl is not opening when purifier open up for overhaul.","E/R - Purifier","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Work in progress, But eventually bowl need to send to workshop to open lock ring on purifer bowl.","2020-02-15"," ","In progress",null,"No","No","No","Internal"]
[null,null,null,null,2120,"83_17/10/2019 6:32:05 PM","2019-10-11","Defect","Ship Staff","Ship Staff Insp.","Main air compressor no-1 and 2 shows signs of crankcase contamination with water, Oil need changing frqently.","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","No-1 main air compressor piston rings replaced and contamination of crankcase oil reduce drastically, also hose connection from crankcase breather to suction filter removed. No-2 compressor piston rings need replacement .","2020-03-15",null,"In progress",null,"No","No","No","Internal"]
[null,null,null,null,8381,"83_Sun Nov 03 2019 01:37:34 GMT+0000 (Coordinated Universal Time)","2019-10-30","Defect","Ship Staff","Ship Staff Insp.","Aux Boiler No 1 and 2 - Gauge glass illumination lights faulty (3 nos)","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Requistion ATHE190197 raised LED light strips. ","2020-04-15",null,"Not Started",null,"No","No","No","Internal"]
[null,null,null,null,8382,"83_Sun Dec 15 2019 10:00:00 GMT+0000 (Coordinated Universal Time)","2019-12-15","Defect","Ship Staff","Ship Staff Insp.","Various wasted pipe support angle bars on main deck.","Deck - Pipe / Fittings","Structural Condn. / WT integrity .","Equipment Related",11.1,"High","Not Applicable","Not Applicable","Temporary repaired.","2020-01-31",null,"Deferred to D D",null,"No","No","No","Internal"]
[null,null,null,null,8383,"83_Sun Dec 15 2019 10:06:29 GMT+0000 (Coordinated Universal Time)","2019-12-15","Defect","Ship Staff","Ship Staff Insp.","Cargo oil tank 2C pressure sensor & Slop-S temperature sensor defective.","Cargo Mach.,Inert Gas","Cargo / Ballast Systems","Equipment Related",8.25,"Very High","Not Applicable","Not Applicable","Can be collorabated with Tank radar K-gauge attendance onboard or Requisition can be raised in Q1/2020","2020-02-05",null,"Not Started",null,"No","No","No","Internal"]
[null,null,null,null,8384,"83_Sun Dec 15 2019 10:10:19 GMT+0000 (Coordinated Universal Time)","2019-12-15","Breakdown,Defect","Ship Staff","Ship Staff Insp.","Pumpromm fix gas detection system screen in the CCR dead.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related",8.4600000000000009,"Very High","Not Applicable","Not Applicable","Waiting spares.","2020-01-25",null,"Waiting spare",null,"No","No","No","Internal"]
[null,null,null,null,8385,"83_15/12/2019 3:51:24 AM","2019-12-15","Defect","Ship Staff","Ship Staff Insp.","Scrubber Tower - High level float alarm was found not fuctioning during routine checks. Found float missing.","Inert Gas","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Requisition ATHE190216 raised and float to be renewed when same received. ","2020-02-15",null,"In progress",null,"No","No","No","Internal"]
[null,null,null,null,8386,"83_15/12/2019 3:55:10 AM","2019-12-15","Defect","Ship Staff","Ship Staff Insp.","ME Local Manoeuvring platform - Telephone booth rotating strobe lights and bell found broken and not fuctional. Same to be replaced.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related",10.37,"Medium","Not Applicable","Not Applicable","Requisition ATHE190218 raised. Same to be renewed when spares received.","2020-02-15",null,"In progress",null,"No","No","No","Internal"]
[null,null,null,null,8387,"83_15/12/2019 8:14:47 PM","2019-12-15","Defect","Ship Staff","Ship Staff Insp.","3pc Air caps missing from location (Forcastle deck-1pc, P/Room COP deck-1pc, Main dk-1)","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","Equipment Related",11.7,"High","Not Applicable","Not Applicable","Req  to be prepared","2020-03-14",null,"Not Started",null,"No","No","No","Internal"]
[null,null,null,null,8388,"83_15/12/2019 8:22:39 PM","2019-12-15","Defect","Ship Staff","Ship Staff Insp.","The indication for the Fire isolation v/v not moving (near 2C). Though the valve is free to operate and it is closing/opeing properly.","LSA / FFA","LSA / FFA Appliances","Equipment Related",5.38,"High","Not Applicable","Not Applicable","To be overhaued the indication mechanism.","2020-02-14",null,"Not Started",null,"No","No","No","Internal"]
[null,null,null,null,null,"83_15/1/2020 4:26:30 AM","2020-01-05","Observation","Ship Staff","Ship Staff Insp.","FORECASTLE DECK WALKWAY TO FOC'LE STORE STANCHION HOLDERS ARE PROVIDED. HOWEVER, STANCHIONS ARE NOT AVAILABLE ONBOARD.","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","Inappropriate Procedure",11.3,"Medium","Not Applicable","Not Applicable","REQUISITION RAISED.","2020-02-05",null,"Waiting spare",null,"No",null,null,"Internal"]
[null,null,null,null,null,"83_15/1/2020 4:34:08 AM","2020-01-11","Breakdown","Ship Staff","Ship Staff Insp.","COP NO.2 AUS SEPARATOR  DP LEVEL TRANSMITTER OUT OF ORDER.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related",8.8000000000000007,"Medium","Not Applicable","Not Applicable","TROUBLESHOOTING IN PROGRESS. TO RAISE REQUISITION.","2020-02-05",null,"Waiting spare",null,"No",null,null,"Internal"]
[null,null,null,null,null,"83_21/1/2020 10:21:30 PM","2019-09-16","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Running hour counter to install for EVAC pumps and record every day.","Cargo Mach.","Eng. / Strg. Comp.","Equipment Related",null,null,"Not Applicable","Not Applicable","Requisition raised ATHE190191","2019-10-16",null,"Waiting spare",null,"No",null,null,"Internal"]
[null,null,null,null,null,"83_21/1/2020 10:27:45 PM","2019-09-16","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Welding curtain is damaged in workshop and need to replace ","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related",5.25,"Medium","Not Applicable","Not Applicable","Requisition raised ATHE190160","2019-10-15",null,"Waiting spare",null,"No",null,null,"Internal"]
[null,null,null,null,null,"83_21/1/2020 10:43:52 PM","2019-09-16","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Salinity and Oil probe on cascade tank is not working, same to order","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related",null,null,"Not Applicable","Not Applicable","Requisition raised ATHE190214","2019-11-15",null,"Waiting spare",null,"No",null,null,"Internal"]
[null,null,null,null,null,"83_22/1/2020 12:15:20 AM","2019-09-16","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","remote control lines for winch operation to be blanked & disconnected. square & round blank to order","Deck - Mooring Machinery","Mooring","Equipment Related",9.17,"High","Not Applicable","Not Applicable","requisition will be raised.","2020-03-31",null,"In progress",null,"No",null,null,"Internal"]

{"sheet":"Completed","index":1,"n_rows":289,"n_cols":28,"rows_kept":289,"cut":false,"hidden":false,"merged":[[10,8,10,9],[10,12,10,13],[12,6,12,27],[8,6,8,27]]}
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,"Defect - Damage Monitoring Sheet"]
[]
[null,null,null,null,null,null,null,"Date of Report","31-11-2019",null,null,"Ship Name","ATHERINA (26-12-2019)"]
[]
[null,null,null,null,null,null,"VERSION : 2.0"]
[]
[]
[]
[null,null,null,null,"ID","UNIQUE ID","Date Recorded","Type of Deficiency","Observer code","Type of Inspection","Description of Deficiency","Equipment Categories","Area of Observation","Deficiency Cause","VIQ Ref Number","Risk Value of Obs","PSC Ref Number","PSC MOU ID","Action Taken or Required","Target Date","PO Ref No.","Status Code","Date Completed","Drydock","Info Sharing","Critical Item","Audit Type","Superintendent Remarks"]
[null,null,null,null,2096,"83_16/10/2019 6:25:12 PM","2019-04-12","Defect","Ship Staff","Ship Staff Insp.","No.1 IG blower main valve getting stuck while opening and requires repair kit and to be overhauled.","Inert Gas","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","New actuator fitted and calibrated and tried out.Found satisfactory. ","2019-09-30",null,"Completed","2019-12-02","No","No","No","Internal"]
[null,null,null,null,2099,"83_16/10/2019 6:30:09 PM","2019-05-15","Defect","Ship Staff","Ship Staff Insp.","IGS Main regulating valve malfunctioning.","Inert Gas","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Electro pneumatic positioner renewed with spare received. Valve tried out. Found satisfactory.","2019-09-30",null,"Completed","2019-12-02","No","No","No","Internal"]
[null,null,null,null,2101,"83_16/10/2019 6:34:09 PM","2019-06-01","Defect","Ship Staff","Ship Staff Insp.","Bunker tank overfill alarm not operational.","Miscellaneous","General Appearance","Equipment Related",10.8,"Medium","Not Applicable","Not Applicable","Defective solenoid replaced with spare new received.Alarm is functional now.","2019-11-15","ATHE190089\t","Completed","2019-10-29","No","No","No","Internal"]
[null,null,null,null,2107,"83_17/10/2019 6:11:57 PM","2019-07-20","Defect","Ship Staff","Ship Staff Insp.","BWTS system CLX1 defective due to water ingress while under operation .","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related",6.22,"Medium","Not Applicable","Not Applicable","Technician attended at USA. Initial setting carried out and system tried out.Working satisfactory.","2019-10-30"," ","Completed","2019-10-22","No","No","No","Internal"]
[null,null,null,null,2110,"83_17/10/2019 6:17:05 PM","2019-08-20","Defect","Ship Staff","Ship Staff Insp.","Rescue boat davit hydraulic pressure dropping very fast, compensator nitrogen bladder bottle seems to be lost nitrogen gas .","LSA / FFA","LSA / FFA Appliances","Equipment Related",5.3,"High","Not Applicable","Not Applicable","Accumulator renewed with new supplied at Kwinana. Davit tried out and found satisfactory.","2019-12-15"," ","Completed","2019-12-14","No","No","No","Internal"]
[null,null,null,null,2122,"83_2019-10-10 20:35:16.000","2019-03-20","Defect","Ship Staff","Ship Staff Insp.","Aconis AMS monitor in ECR console are not original and fitted with normal PC monitor.\t","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Original monitor ordered and fixed","2019-04-30","ATHE195060","Completed","2019-04-24","No","No","No","Internal"]
[null,null,null,null,2123,"83_2019-11-10 01:29:21.000","2019-04-10","Defect","Ship Staff","Ship Staff Insp.","Steering gear No 1 pp having oil leak from pp block. Need to check leak location.\t\t","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related",10.39,"High","Not Applicable","Not Applicable","Pump casing block tightened and found no leak on the pump side.","2019-04-30",null,"Completed","2019-04-24","No","No","No","Internal"]
[null,null,null,null,2124,"83_2019-10-11 01:33:07.000","2019-04-09","Defect","Ship Staff","Ship Staff Insp.","ME fuel oil fine filter change over mechanism hard.\t","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Change over mechanism overhauled and now its working satisfactory.","2019-04-15",null,"Completed","2019-04-10","No","No","No","Internal"]
[null,null,null,null,2125,"83_2019-11-10 01:36:16.000","2019-03-30","Defect","Ship Staff","Ship Staff Insp.","Dust in many electric panels. Many contacts causing low insulation alarm. To clean them and order spares contacts.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related",10.37,"Medium","Not Applicable","Not Applicable","MSBD and AMS panel cleaning carried out at yard. Spare contactors ordered.","2019-04-10","ATHE195030","Completed","2019-04-04","No","No","No","Internal"]
[null,null,null,null,2126,"83_2019-11-10 01:38:36.000","2019-04-12","Defect","Ship Staff","Ship Staff Insp.","IG panel turn switch malfuntion. Presently wire disconnected.","Inert Gas","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Switch repaired and its function check carried out.","2019-04-15",null,"Completed","2019-04-14","No","No","No","Internal"]
[null,null,null,null,2127,"83_2019-11-10 01:41:57.999","2019-04-02","Defect","Ship Staff","Ship Staff Insp.","Residual BN and Iron to measure and OBSERVE the liner surface. LO test kit to order.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related",10.7,"Medium","Not Applicable","Not Applicable","Test kit received and samples send for shore analysis. Onboard test to be carried out shortly.","2019-04-29",null,"Completed","2019-04-29","No","No","No","Internal"]
[null,null,null,null,2128,"83_2019-11-10 01:46:10.000","2019-03-30","Defect","Ship Staff","Ship Staff Insp.","Hydraulic top bracing FWD leaking when charging oil. Suspect cylinder seal damaged and require replacement.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Gas changed in accumulator. As off now no leak is observed and have 1set of seals as spares.","2019-05-30",null,"Completed","2019-04-25","No","No","No","Internal"]
[null,null,null,null,2129,"83_2019-11-10 01:49:41.999","2019-04-12","Defect","Ship Staff","Ship Staff Insp.","ME lub oil sump to top up with 6000 litres of oil as presently level around 36,000 ltr.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Sump oil topped up with 6500 litres.","2019-04-15",null,"Completed","2019-04-13","No","No","No","Internal"]
[null,null,null,null,2130,"83_2019-11-10 01:51:39.000","2019-03-30","Defect","Ship Staff","Ship Staff Insp.","DG No.3 exhaust gas temp A sensor to be replaced.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Sensor replaced with spare new sensor.","2019-04-25",null,"Completed","2019-04-25","No","No","No","Internal"]
[null,null,null,null,2131,"83_2019-11-10 01:54:46.000","2019-04-08","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","No recovery unit / pump - bottles for Main ac for collecting gas.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Received at call singapore","2019-04-25",null,"Completed","2019-04-23","No","No","No","Internal"]
[null,null,null,null,2132,"83_2019-11-10 01:56:41.999","2019-03-17","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","WECS computer for wartisila need to upgrade.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Upgraded with new software and hardware.","2019-04-25",null,"Completed","2019-04-23","No","No","No","Internal"]
[null,null,null,null,2133,"83_2019-11-10 01:58:31.999","2019-03-21","Defect","Ship Staff","Ship Staff Insp.","Engine performance system for AE and ME","E/R - Aux. Engine,E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","ME and DG performance taken.","2019-04-26",null,"Completed","2019-04-26","No","No","No","Internal"]
[null,null,null,null,2134,"83_2019-11-10 14:49:52.000","2019-04-05","Defect","Ship Staff","Ship Staff Insp.","Damaged and Oil soaked lagging to be replaced in some loacations in the Engine room.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related",10.29,"Medium","Not Applicable","Not Applicable","All damaged laggings replaced with spare laggings.","2019-04-25",null,"Completed","2019-04-25","No","No","No","Internal"]
[null,null,null,null,2135,"83_2019-11-10 14:52:04.999","2019-03-28","Defect","Ship Staff","Ship Staff Insp.","IG additional O2 panel installation ( MESQAC requirement)","Inert Gas","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","New O2 panel installed with all the fittings.","2019-04-25",null,"Completed","2019-04-18","No","No","No","Internal"]
[null,null,null,null,2136,"83_2019-11-10 14:54:31.000","2019-04-03","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Boiler and Composite boilers need service engineers to check the settings for IG and water level controllers.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Kangrim service Engineers attended at singapore. Both Aux. boilers are operating satisfactory.","2019-04-25",null,"Completed","2019-04-22","No","No","No","Internal"]
[null,null,null,null,2137,"83_2019-11-10 14:56:41.000","2019-04-07","Defect","Ship Staff","Ship Staff Insp.","Emergency generator cooling water pressure switch bypassed.","Elect. Mach. & Equip.","Emgcy. Systems","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Pressure switch renewed.","2019-04-25",null,"Completed","2019-04-24","No","No","No","Internal"]
[null,null,null,null,2138,"83_2019-11-10 15:02:49.999","2019-04-05","Defect","Ship Staff","Ship Staff Insp.","Hot water calorifier steam heater body gasket leaking.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related",10.29,"Medium","Not Applicable","Not Applicable","Gasket renewed. No leaks in the system.","2019-04-10",null,"Completed","2019-04-05","No","No","No","Internal"]
[null,null,null,null,2139,"83_2019-10-11 15:05:18.000","2019-04-02","Defect","Ship Staff","Ship Staff Insp.","Blue line bulkhead master valve suspect passing.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related",8.11,"High","Not Applicable","Not Applicable","RO received, Job completed.","2019-04-15","ATHE195057","Completed","2019-04-12","No","No","No","Internal"]
[null,null,null,null,2140,"83_2019-11-10 15:12:40.000","2019-04-10","Defect","Ship Staff","Ship Staff Insp.","440 Volt alarm due to low insulation from ER vent fan and Boiler no:1 panel. Need investigation.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related",10.38,"Medium","Not Applicable","Not Applicable","Boiler No:1 faulty contactor replaced and ER vent fan naked wire insulated. 440V insulation meter shows now infinity.","2019-04-13",null,"Completed","2019-04-11","No","No","No","Internal"]
[null,null,null,null,2141,"83_2019-11-10 15:15:09.000","2019-04-22","Defect","Ship Staff","Ship Staff Insp.","Emergency fire pump not building pressure.","Critical Equip.","Eng. / Strg. Comp.","Equipment Related",5.41,"Very High","Not Applicable","Not Applicable","Priming pump engaging lever found broken, same welded. Pump tried out and found to be woeking satisfactory.","2019-04-23",null,"Completed","2019-04-23","No","No","No","Internal"]
[null,null,null,null,2142,"83_2019-10-11 15:27:32.000","2019-04-22","Defect","Ship Staff","Ship Staff Insp.","OWS 3-way valve malfunctioning on test mode.","Critical Equip.","Eng. / Strg. Comp.","Equipment Related",6.17,"Very High","Not Applicable","Not Applicable","Complete unit replaced by the shore w/shop UNI Marine services Singapore ( Cell + Calib.unit). Tried out and found to be working.","2019-04-23",null,"Completed","2019-04-23","No","No","No","Internal"]
[null,null,null,null,2143,"83_2019-11-10 15:38:20.000","2019-04-24","Defect","Ship Staff","Ship Staff Insp.","Bilge pump not taking suc.properly.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related",6.14,"High","Not Applicable","Not Applicable","Assy.dismantled. Valve and valve seat having piting marks , same build up by steel putty and lapped. Pump tried out-working ok.","2019-04-24",null,"Completed","2019-04-24","No","No","No","Internal"]
[null,null,null,null,2144,"83_2019-12-10 03:44:30.000","2019-03-08","Defect","Ship Staff","Ship Staff Insp.","OWS ist stage filter fully wasted/oil soaked","Critical Equip.","Eng. / Strg. Comp.","Equipment Related",6.17,"Very High","Not Applicable","Not Applicable","First stage filter replaced with the spare one.","2019-04-30",null,"Completed","2019-04-24","No","No","No","Internal"]
[null,null,null,null,2145,"83_2019-12-10 03:46:20.000","2019-03-20","Defect","Ship Staff","Ship Staff Insp.","Fire bilge and GS pump No.1 Mechanical seal leaking.","LSA / FFA","Eng. / Strg. Comp.","Equipment Related",5.38,"High","Not Applicable","Not Applicable","Mech.seal replaced with the spare one.","2019-04-30",null,"Completed","2019-04-25","No","No","No","Internal"]
[null,null,null,null,2146,"83_2019-10-12 03:47:47.000","2019-04-25","Defect","Ship Staff","Ship Staff Insp.","Air.cond.compressor no.2 mech.seal leaking.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Mech.seal replaced with the spare one.","2019-04-27",null,"Completed","2019-04-25","No","No","No","Internal"]
[null,null,null,null,2147,"83_2019-12-10 03:49:10.000","2019-04-12","Defect","Ship Staff","Ship Staff Insp.","DG 2 fuel filter leaking oil from top.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related",10.19,"Very High","Not Applicable","Not Applicable","Leakage rectified.","2019-04-30",null,"Completed","2019-04-26","No","No","No","Internal"]
[null,null,null,null,2148,"83_2019-12-10 03:52:13.000","2019-03-30","Defect","Ship Staff","Ship Staff Insp.","IG scrubber high level float alarm erratic and temporarily repaired.","Inert Gas","Eng. / Strg. Comp.","Equipment Related",8.25,"Very High","Not Applicable","Not Applicable","High level float renewed and tried out-satisfactory.","2019-04-30",null,"Completed","2019-04-26","No","No","No","Internal"]
[null,null,null,null,2149,"83_2019-12-10 03:53:58.000","2019-04-05","Defect","Ship Staff","Ship Staff Insp.","Incinerator refractory to order. Sludge burning to start in incinrateor.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related",6.16,"Very High","Not Applicable","Not Applicable","Refractory is in good condition. Sludge burning started in incinerator.","2019-04-28",null,"Completed","2019-04-26","No","No","No","Internal"]
[null,null,null,null,2150,"83_2019-12-10 03:55:40.000","2019-03-20","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Graviner oil mist detector EPROM and software upgrade.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related",10.210000000000001,"Medium","Not Applicable","Not Applicable","monitoring and no issues till now. ","2019-05-30",null,"Completed","2019-04-26","No","No","No","Internal"]
[null,null,null,null,2151,"83_2019-12-10 03:58:05.999","2019-04-12","Defect","Ship Staff","Ship Staff Insp.","Inert gas temp found to be going higher withing short period of operation.","Inert Gas","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Scruuber tower all nozzles removed and cleared off dirt/sea shells.","2019-05-30",null,"Completed","2019-04-26","No","No","No","Internal"]
[null,null,null,null,2152,"83_2019-10-12 04:00:27.999","2019-04-02","Defect","Ship Staff","Ship Staff Insp.","4C COT Stripper valve passing.","Deck - Machinery","Cargo / Ballast Systems","Equipment Related",8.11,"Medium","Not Applicable","Not Applicable","Seat ring  renewed","2019-04-16","ATHE195057","Completed","2019-04-16","No","No","No","Internal"]
[null,null,null,null,2153,"83_2019-12-10 05:02:49.999","2019-04-12","Defect","Ship Staff","Ship Staff Insp.","Kongsberg System Max. depths for all centre tanks needs to be corrected  noted a difference in the Max. depths in the sounding tables and the actual on board.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related",8.1300000000000008,"Medium","Not Applicable","Not Applicable","Kongberg technician needed to attend the same // SERVICE ENGR ATTENDED AT SINGAPORE ON 22 APR. FAULT RECTIFIED.","2019-04-22",null,"Completed","2019-04-22","No","No","No","Internal"]
[null,null,null,null,2154,"83_2019-12-10 05:09:10.000","2019-04-12","Defect","Ship Staff","Ship Staff Insp.","Ballast Sea chest Valve cannot be opened from the Cargo Control Room. Need to open / shut using hand pump.","Deck - Machinery","Eng. / Strg. Comp.","Equipment Related",8.11,"Medium","Not Applicable","Not Applicable","Technician in singapore attended // FAULT RECTIFIED.","2019-04-22",null,"Completed","2019-04-22","No","No","No","Internal"]
[null,null,null,null,2155,"83_2019-12-10 06:14:42.000","2019-04-02","Defect","Ship Staff","Ship Staff Insp.","Cargo and Bunker Overfill alarm hooters on deck not working. ","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related",8.14,"Very High","Not Applicable","Not Applicable","RO Raised, spares received at Canaport, deck overfill alarm hooters working, bunker overfill alarm hooter remains ATHE190089.","2019-04-22","ATHE190033 & ATHE190089","Completed","2019-04-22","No","No","No","Internal"]
[null,null,null,null,2156,"83_2019-12-10 06:17:20.000","2019-04-02","Defect","Ship Staff","Ship Staff Insp.","Both pilot ladders not solas approved.\t\t","LSA / FFA","LSA / FFA Appliances","Equipment Related",5.47,"Medium","Not Applicable","Not Applicable","RO RECEIVED,  NEW PILOT LADDER  RECEIVED & IN USE.","2019-04-22","ATHE195079","Completed","2019-04-22","No","No","No","Internal"]
[null,null,null,null,2157,"83_2019-12-10 06:19:04.999","2019-04-02","Defect","Ship Staff","Ship Staff Insp.","6 Nos Mandal shackle need renewal, Found wasted.","Deck - Machinery","General Appearance","Equipment Related",9.17,"High","Not Applicable","Not Applicable","NEW MANDAL SHACKLE RECEIVED & RENEWED.","2019-04-22","ATHE190031","Completed","2019-04-22","No","No","No","Internal"]
[null,null,null,null,2158,"83_2019-12-10 06:26:08.000","2019-04-12","Defect","Ship Staff","Ship Staff Insp.","NO.2 BALLAST PUMP DISCHARGE PRESSURE TRANSMITTER SHOWING PRESSURE BUT ACTUAL ITS ZERO","Elect. Mach. & Equip.","Cargo / Ballast Systems","Equipment Related",8.8000000000000007,"Medium","Not Applicable","Not Applicable","Pressure transmitter changed, working satisfactory.","2019-04-19",null,"Completed","2019-04-19","No","No","No","Internal"]
[null,null,null,null,2159,"83_2019-12-10 06:29:24.000","2019-04-12","Defect","Ship Staff","Ship Staff Insp.","Cargo seachest valve not fitted with regulator.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related",8.11,"Medium","Not Applicable","Not Applicable","REGULATOR RECEIVED & RENEWED.","2019-04-22","ATHE195090","Completed","2019-04-22","No","No","No","Internal"]
[null,null,null,null,2160,"83_2019-12-10 06:31:34.000","2019-04-12","Defect","Ship Staff","Ship Staff Insp.","1S COT Overfill alarm float stuck.\t","Elect. Mach. & Equip.","Cargo / Ballast Systems","Equipment Related",8.14,"Very High","Not Applicable","Not Applicable","overhauled & Working satisfactory after overhaul. ","2019-04-16",null,"Completed","2019-04-16","No","No","No","Internal"]
[null,null,null,null,2161,"83_2019-12-10 06:32:58.999","2019-04-12","Defect","Ship Staff","Ship Staff Insp.","Cargo, Ballast, Pumproom valves indicators showing erratic.\t","Elect. Mach. & Equip.","Cargo / Ballast Systems","Equipment Related",8.11,"Medium","Not Applicable","Not Applicable","overhauled & Working satisfactory after overhaul. ","2019-04-23",null,"Completed","2019-04-23","No","No","No","Internal"]
[null,null,null,null,2162,"83_2019-12-10 06:32:24.000","2019-04-02","Defect","Ship Staff","Ship Staff Insp.","Slop s COT Valve passing.","Deck - Machinery","Cargo / Ballast Systems","Equipment Related",8.11,"Medium","Not Applicable","Not Applicable","Seat ring renewed.","2019-04-28","ATHE195057","Completed","2019-04-30","No","No","No","Internal"]
[null,null,null,null,2163,"83_2019-10-12 06:33:47.000","2019-04-22","Defect","Ship Staff","Ship Staff Insp.","Oil traces found in the observation tank.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Main engine fuel oil heater no.2 found 1no tube leaking,same plugged.Again pr.tested and observed no leaks.We will keep monitoring.","2019-05-30",null,"Completed","2019-05-02","No","No","No","Internal"]
[null,null,null,null,2164,"83_2019-12-10 06:35:56.999","2019-05-01","Defect","Ship Staff","Ship Staff Insp.","FWG dosing pump non functional.","E/R - Aux. Mach.","Emgcy. Systems","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Pump dismantled ,inspected and all parts cleaned.Discharge line found clogged,same cleared.","2019-05-10",null,"Completed","2019-05-03","No","No","No","Internal"]
[null,null,null,null,2165,"83_2019-12-10 06:37:40.000","2019-05-01","Defect","Ship Staff","Ship Staff Insp.","Main engine booster pump no.2 not building sufficient pressure.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Fault traced with the relief valve.Same dismantled, o'hauled and relief v/v adjusted.","2019-05-12",null,"Completed","2019-05-04","No","No","No","Internal"]
[null,null,null,null,2166,"83_2019-12-10 06:39:06.000","2019-04-02","Defect","Ship Staff","Ship Staff Insp.","VECS System pressure guage not working in CCR.","Elect. Mach. & Equip.","Emgcy. Systems","Equipment Related",8.25,"Very High","Not Applicable","Not Applicable","This was due to wrong connections given in shipyard,same rectified.","2019-05-10",null,"Completed","2019-05-07","No","No","No","Internal"]
[null,null,null,null,2167,"83_2019-12-10 06:40:59.000","2019-04-21","Defect","Ship Staff","Ship Staff Insp.","Stbd Windlass Brake Cylinder leaking.","Deck - Mooring Machinery","Mooring","Equipment Related",9.1999999999999993,"Medium","Not Applicable","Not Applicable","Seals renewed.Brake cyl.tested and observed no leaks .","2019-05-05",null,"Completed","2019-05-07","No","No","No","Internal"]
[null,null,null,null,2168,"83_2019-12-10 06:42:22.000","2019-04-12","Defect","Ship Staff","Ship Staff Insp.","7 Nos. Foam Monitor valves leaking. ","LSA / FFA","General Appearance","Equipment Related",5.38,"High","Not Applicable","Not Applicable","Valves renewed.","2019-05-06","ATHE190037","Completed","2019-05-09","No","No","No","Internal"]
[null,null,null,null,2169,"83_2019-12-10 06:44:50.000","2019-04-02","Defect","Ship Staff","Ship Staff Insp.","2P WBT Main valve passing.","Deck - Pipe / Fittings","General Appearance","Equipment Related",8.11,"Medium","Not Applicable","Not Applicable","Valve seat ring renewed.","2019-05-13",null,"Completed","2019-05-11","No","No","No","Internal"]
[null,null,null,null,2170,"83_2019-12-10 06:46:34.000","2019-05-06","Defect","Ship Staff","Ship Staff Insp.","Hydraulic leak in MW6 Winch remote opeartion pressure line .","Deck - Mooring Machinery","Mooring","Equipment Related",9.14,"Medium","Not Applicable","Not Applicable","Leakage rectified.","2019-05-13",null,"Completed","2019-05-14","No","No","No","Internal"]
[null,null,null,null,2171,"83_2019-12-10 06:48:52.000","2019-04-10","Defect","Ship Staff","Ship Staff Insp.","Stbd windlass Hyd cylinder for engaing / disengaging gear is not working.","Deck - Mooring Machinery","Mooring","Equipment Related",9.1999999999999993,"Medium","Not Applicable","Not Applicable","Hyd.cylinder eased up and found to working satisfactory.","2019-07-08",null,"Completed","2019-05-14","No","No","No","Internal"]
[null,null,null,null,2172,"83_2019-12-10 06:50:29.000","2019-05-14","Defect","Ship Staff","Ship Staff Insp.","Hydraulic leak in MW2 Winch remote opeartion pressure line.","Deck - Mooring Machinery","Mooring","Equipment Related",9.14,"Medium","Not Applicable","Not Applicable","Leakage rectified.","2019-05-16",null,"Completed","2019-05-15","No","No","No","Internal"]
[null,null,null,null,2173,"83_2019-12-10 06:53:02.000","2019-04-23","Defect","Ship Staff","Ship Staff Insp.","No.2 Ballast pump suction guage found inoperational.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related",8.8000000000000007,"Medium","Not Applicable","Not Applicable","Suction gauge repaired  & Working satisfactory after overhaul. ","2019-05-14",null,"Completed","2019-05-15","No","No","No","Internal"]
[null,null,null,null,2174,"83_2019-12-10 06:54:46.000","2019-05-16","Defect","Ship Staff","Ship Staff Insp.","Composite boiler feed water pump no.2 mech.seal leaking.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Pump and motor o'hauled.Tried out-all in order.","2019-05-17",null,"Completed","2019-05-16","No","No","No","Internal"]
[null,null,null,null,2175,"83_2019-12-10 06:56:04.000","2019-05-16","Defect","Ship Staff","Ship Staff Insp.","DGs fuel oil heater no.2 relief valve leaking.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related",10.29,"Medium","Not Applicable","Not Applicable","Relief valve dismantled,inspected and all parts cleaned.Heater put back in use and found no leaks.","2019-05-20",null,"Completed","2019-05-18","No","No","No","Internal"]
[null,null,null,null,2176,"83_2019-12-10 06:57:18.000","2019-04-02","Defect","Ship Staff","Ship Staff Insp.","SEVERAL WHEELS FOR COW MACHINE VALVE & FIRE LINE FOUND BROKEN & DAMAGED.\t\t","Cargo Mach.","Cargo / Ballast Systems","Equipment Related",8.11,"Medium","Not Applicable","Not Applicable","All renewed","2019-05-20",null,"Completed","2019-05-18","No","No","No","Internal"]
[null,null,null,null,2177,"83_14/10/2019 5:54:41 PM","2019-04-10","Defect","Ship Staff","Ship Staff Insp.","No.2 COP Discharge NRV (750 A) leaking from flange. Gasket for same needs to be replaced.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related",8.11,"Medium","Not Applicable","Not Applicable","Gasket need to be renewed , flange need to be tighten.","2019-05-18",null,"Completed","2019-05-16","No","No","No","Internal"]
[null,null,null,null,2178,"83_14/10/2019 5:55:52 PM","2019-04-12","Defect","Ship Staff","Ship Staff Insp.","Port gangway collapsable rail 4 stanchions found damaged.","LSA / FFA","LSA / FFA Appliances","Equipment Related",5.47,"Medium","Not Applicable","Not Applicable","fabricated & renewed.","2019-05-18",null,"Completed","2019-05-20","No","No","No","Internal"]
[null,null,null,null,2179,"83_14/10/2019 5:57:19 PM","2019-05-18","Defect","Ship Staff","Ship Staff Insp.","Fwd hyd.system no.3 pump discharge hose raptured.","Deck - Mooring Machinery","Mooring","Equipment Related",9.14,"Medium","Not Applicable","Not Applicable","Hose replaced  with the spare one.","2019-07-30",null,"Completed","2019-05-18","No","No","No","Internal"]
[null,null,null,null,2180,"83_14/10/2019 5:59:18 PM","2019-05-19","Defect","Ship Staff","Ship Staff Insp.","HFO Purifier no.2 heater steam side gasket leaking.","E/R - Purifier","Eng. / Strg. Comp.","Equipment Related",10.29,"Medium","Not Applicable","Not Applicable","Gasket renewed. No leaks in the system.","2019-05-25",null,"Completed","2019-05-21","No","No","No","Internal"]
[null,null,null,null,2181,"83_14/10/2019 6:04:31 PM","2019-04-02","Defect","Ship Staff","Ship Staff Insp.","AC controller fluctiaing and suspect PCB will fail in due course. Other PCB already renenwed recently.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Spare PCB ordered and received on board, kept as spare . Old PCB working satisfactory after cleaning PCB and wiring connections retighten.","2019-07-10",null,"Completed","2019-05-21","No","No","No","Internal"]
[null,null,null,null,2182,"83_14/10/2019 6:06:05 PM","2019-03-27","Defect","Ship Staff","Ship Staff Insp.","Observation tank level gauge glass found to be broken at the top side.\t","Miscellaneous","Eng. / Strg. Comp.","Equipment Related",10.25,"Very High","Not Applicable","Not Applicable","Gauge glass renewed","2019-06-01",null,"Completed","2019-05-21","No","No","No","Internal"]
[null,null,null,null,2183,"83_14/10/2019 6:08:27 PM","2019-04-12","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Hyd block / directional valve for mooring winch to order .","Deck - Mooring Machinery","Mooring","Equipment Related",9.14,"Medium","Not Applicable","Not Applicable","Spares  ordered and repaired carry out on leaky blocks, presently no leaks.","2019-07-10","ATHE190048","Completed","2019-05-21","No","No","No","Internal"]
[null,null,null,null,2184,"83_14/10/2019 6:10:27 PM","2019-04-12","Defect","Ship Staff","Ship Staff Insp.","Ballast pp no 2 lower mech seal lekaing.\t","Cargo Mach.","Cargo / Ballast Systems","Equipment Related",8.8000000000000007,"Medium","Not Applicable","Not Applicable","No leaks observed during loading at Juaymah.","2019-07-10",null,"Completed","2019-05-22","No","No","No","Internal"]
[null,null,null,null,2185,"83_14/10/2019 6:11:48 PM","2019-04-03","Defect","Ship Staff","Ship Staff Insp.","Pressure transmitter (oil and suction)  of AC 2 plant temporarily repaired.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","It is working ok .Will replace as required.","2019-07-10",null,"Completed","2019-05-22","No","No","No","Internal"]
[null,null,null,null,2186,"83_14/10/2019 6:13:56 PM","2019-05-23","Defect","Ship Staff","Ship Staff Insp.","Main engine L.O.Pump no.2 MCB tripping  during star/delta c/o.\t","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Fault traced with the  delta contactor,same contacts cleaned.Pump put into operation and found to be working satisfactory.","2019-05-23",null,"Completed","2019-05-23","No","No","No","Internal"]
[null,null,null,null,2187,"83_14/10/2019 6:15:42 PM","2019-05-24","Defect","Ship Staff","Ship Staff Insp.","Bunker tanks common steam return line flange gasket leaking.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related",10.29,"Medium","Not Applicable","Not Applicable","Gasket renewed. ","2019-05-24",null,"Completed","2019-05-24","No","No","No","Internal"]
[null,null,null,null,2188,"83_14/10/2019 6:18:11 PM","2019-04-02","Defect","Ship Staff","Ship Staff Insp.","Air conditon plant solenoid valve for compressor oil return malfunction.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Solenoid valve replaced.","2019-07-01",null,"Completed","2019-05-24","No","No","No","Internal"]
[null,null,null,null,2189,"83_14/10/2019 6:19:38 PM","2019-04-01","Defect","Ship Staff","Ship Staff Insp.","DG 3 LO priming pp motor making noise. Require replacement. Spare motor onboard.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Pump and motor decoupled,inspected.Motor o'hauled and tried out-satisfactory.","2019-06-30",null,"Completed","2019-05-25","No","No","No","Internal"]
[null,null,null,null,2190,"83_14/10/2019 6:20:51 PM","2019-05-23","Defect","Ship Staff","Ship Staff Insp.","13 Nos PV Valve leaking from Vaccum & pressure side.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related",8.4,"Medium","Not Applicable","Not Applicable","PV Valves overhauled.","2019-06-05",null,"Completed","2019-05-30","No","No","No","Internal"]
[null,null,null,null,2191,"83_14/10/2019 6:22:08 PM","2019-04-01","Defect","Ship Staff","Ship Staff Insp.","Galley out of 4 plates 2 are working normal.","Elect. Mach. & Equip.","General Appearance","Equipment Related",10.37,"Medium","Not Applicable","Not Applicable","2 no.hot plates renewed and working satisfactory.","2019-07-01",null,"Completed","2019-05-30","No","No","No","Internal"]
[null,null,null,null,2192,"83_14/10/2019 6:24:06 PM","2019-04-25","Defect","Ship Staff","Ship Staff Insp.","Pumproom davit found freezed, not swinging.","Deck - Machinery","General Appearance","Equipment Related",8.5,"Medium","Not Applicable","Not Applicable","Overhauled, greased & freed.","2019-05-30",null,"Completed","2019-05-31","No","No","No","Internal"]
[null,null,null,null,2193,"83_14/10/2019 6:25:32 PM","2019-04-14","Defect","Ship Staff","Ship Staff Insp.","Few strands for pumproom davit wire found broken.","Deck - Machinery","General Appearance","Equipment Related",8.5,"Medium","Not Applicable","Not Applicable","Wire  renewed.","2019-06-02",null,"Completed","2019-06-01","No","No","No","Internal"]
[null,null,null,null,2194,"83_14/10/2019 6:26:50 PM","2019-04-21","Defect","Ship Staff","Ship Staff Insp.","Yellow & Blue line AUS pneumatic discharge valve showing partially open in CCR, But actual in local the valve is fully closed.","Deck - Pipe / Fittings","General Appearance","Equipment Related",8.11,"Medium","Not Applicable","Not Applicable","purged & adjusted, working well.","2019-06-03",null,"Completed","2019-06-05","No","No","No","Internal"]
[null,null,null,null,2195,"83_14/10/2019 6:28:17 PM","2019-05-24","Defect","Ship Staff","Ship Staff Insp.","5C & 5S COT IG Pressure in Tank radar system : 5S showing pressure for 5C & Vice a versa.\t","Inert Gas","Cargo / Ballast Systems","Equipment Related",8.1300000000000008,"Medium","Not Applicable","Not Applicable","Wiring on 5C and 5S checked/ interchanged and now working satisfactory, It was wiring fault which was rectified. ","2019-06-05",null,"Completed","2019-06-04","No","No","No","Internal"]
[null,null,null,null,2196,"83_14/10/2019 6:43:08 PM","2019-05-23","Defect","Ship Staff","Ship Staff Insp.","3C COT IG Pressure sensor showing erratic reading.","Inert Gas","Cargo / Ballast Systems","Equipment Related",8.1300000000000008,"Medium","Not Applicable","Not Applicable","3C COT IG pressure sensor terminals cleaned in electronic unit - now working satisfactory. ","2019-06-05",null,"Completed","2019-06-04","No","No","No","Internal"]
[null,null,null,null,2197,"83_14/10/2019 6:44:44 PM","2019-06-01","Defect","Ship Staff","Ship Staff Insp.","3P WBT Sounding pipe cap found wasted.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related",8.8000000000000007,"Medium","Not Applicable","Not Applicable"," fabricated & renewed.","2019-06-08",null,"Completed","2019-06-06","No","No","No","Internal"]
[null,null,null,null,2198,"83_14/10/2019 6:46:09 PM","2019-06-02","Defect","Ship Staff","Ship Staff Insp.","Emergency fire pump mech.seal leaking.","LSA / FFA","Emgcy. Systems","Equipment Related",5.38,"High","Not Applicable","Not Applicable","Mech.seal,mech.seal cover o-ring and oil seal replaced.Pump tried out-all in order.","2019-06-04",null,"Completed","2019-06-04","No","No","No","Internal"]
[null,null,null,null,2199,"83_14/10/2019 6:47:40 PM","2019-06-03","Defect","Ship Staff","Ship Staff Insp.","Inert gas system scrubber cooling sea water pump mech.seal leaking.","Inert Gas","Eng. / Strg. Comp.","Equipment Related",10.31,"Very High","Not Applicable","Not Applicable","Mech.seal,mech.seal cover o-ring and carbon metal replaced.Pump tried out-all in order.","2019-06-08",null,"Completed","2019-06-05","No","No","No","Internal"]
[null,null,null,null,2200,"83_14/10/2019 6:49:34 PM","2019-03-10","Defect","Ship Staff","Ship Staff Insp.","Engine room crane wire needs  renewal.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related",10.28,"Low","Not Applicable","Not Applicable","Wire renewed on 7th Apr 2019, job completed.","2019-06-20",null,"Completed","2019-04-07","No","No","No","Internal"]
[null,null,null,null,2201,"83_14/10/2019 6:51:21 PM","2019-04-12","Defect","Ship Staff","Ship Staff Insp.","AE Purifier inoperative due to leaky sol.","E/R - Purifier","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Solenoids repalced and purifier working satisfactory.","2019-07-10",null,"Completed","2019-06-06","No","No","No","Internal"]
[null,null,null,null,2202,"83_14/10/2019 6:52:48 PM","2019-03-13","Defect","Ship Staff","Ship Staff Insp.","Sewage holding tank level gauge inoperative .","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Gauge renewed.","2019-07-30",null,"Completed","2019-06-09","No","No","No","Internal"]
[null,null,null,null,2203,"83_14/10/2019 6:54:22 PM","2019-06-08","Defect","Ship Staff","Ship Staff Insp.","Stripper pump gland packing leaking.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related",8.8000000000000007,"Medium","Not Applicable","Not Applicable","renewed.","2019-06-12",null,"Completed","2019-06-10","No","No","No","Internal"]
[null,null,null,null,2204,"83_14/10/2019 6:55:32 PM","2019-05-20","Defect","Ship Staff","Ship Staff Insp.","NO.3 COP Separator drain line found holed.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related",8.8000000000000007,"Medium","Not Applicable","Not Applicable","Fabricated & renewed.","2019-06-05",null,"Completed","2019-06-10","No","No","No","Internal"]
[null,null,null,null,2205,"83_14/10/2019 7:00:30 PM","2019-03-23","Defect","Ship Staff","Ship Staff Insp.","DG3 Air starting reducing valve malfunctioning.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Reducing valve o'hauled and operating satisfactory .","2019-06-25",null,"Completed","2019-06-10","No","No","No","Internal"]
[null,null,null,null,2206,"83_14/10/2019 7:03:33 PM","2019-04-22","Defect","Ship Staff","Ship Staff Insp.","Boiler fuel oil pump no 2 not building sufficient pressure .","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Pump replaced with a new one .","2019-06-30",null,"Completed","2019-06-10","No","No","No","Internal"]
[null,null,null,null,2207,"83_15/10/2019 10:23:10 AM","2019-05-07","Defect","Ship Staff","Ship Staff Insp.","Deck seal pump no 1 mech seal leaking.","Inert Gas","Eng. / Strg. Comp.","Equipment Related",10.31,"Very High","Not Applicable","Not Applicable","Pump shaft casing rings,mech.seal and shaft renewed.","2019-07-03",null,"Completed","2019-06-11","No","No","No","Internal"]
[null,null,null,null,2208,"83_15/10/2019 10:24:14 AM","2019-04-25","Defect","Ship Staff","Ship Staff Insp.","Valve remote system 3no.pressure switches faulty.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related",8.8000000000000007,"Medium","Not Applicable","Not Applicable","Pressure switches replaced.","2019-06-30",null,"Completed","2019-06-11","No","No","No","Internal"]
[null,null,null,null,2209,"83_15/10/2019 10:25:26 AM","2019-04-10","Defect","Ship Staff","Ship Staff Insp.","Alarm monitoring system diode defective.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related",10.37,"Medium","Not Applicable","Not Applicable","Diode renewed.","2019-06-30",null,"Completed","2019-06-11","No","No","No","Internal"]
[null,null,null,null,2210,"83_15/10/2019 10:26:49 AM","2019-04-12","Defect","Ship Staff","Ship Staff Insp.","Air filter to install in the new IG  oxygen sensor line.","Inert Gas","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Filter installed.","2019-06-01",null,"Completed","2019-06-12","No","No","No","Internal"]
[null,null,null,null,2211,"83_15/10/2019 10:28:15 AM","2019-05-05","Defect","Ship Staff","Ship Staff Insp.","Incinerator dosing pump mech. seal leaking.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Pump replaced with a new one.","2019-06-30",null,"Completed","2019-06-12","No","No","No","Internal"]
[null,null,null,null,2212,"83_15/10/2019 10:29:33 AM","2019-04-15","Defect","Ship Staff","Ship Staff Insp.","B/R window wiper no.5 motor needs renewal.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related",11.9,null,"Not Applicable","Not Applicable","Wiper motor renewed.","2019-06-30",null,"Completed","2019-06-14","No","No","No","Internal"]
[null,null,null,null,2213,"83_15/10/2019 10:30:53 AM","2019-06-14","Defect","Ship Staff","Ship Staff Insp.","Fwd Winch Hydraulic cooling line found holed.","Deck - Mooring Machinery","Mooring","Equipment Related",9.14,"Medium","Not Applicable","Not Applicable","fabricated & renewed.","2019-06-20",null,"Completed","2019-06-15","No","No","No","Internal"]
[null,null,null,null,2214,"83_15/10/2019 10:32:07 AM","2019-06-14","Defect","Ship Staff","Ship Staff Insp."," 7 Fire hydrant found leaking.","LSA / FFA","LSA / FFA Appliances","Equipment Related",5.38,"High","Not Applicable","Not Applicable","Fire hydrant valve overhauled & renewed.","2019-06-20",null,"Completed","2019-06-17","No","No","No","Internal"]
[null,null,null,null,2215,"83_15/10/2019 10:33:20 AM","2019-06-08","Defect","Ship Staff","Ship Staff Insp.","ME Rpm detector system 2,no.1 pick up sensor faulty.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Sensor replaced.","2019-06-20",null,"Completed","2019-06-17","No","No","No","Internal"]
[null,null,null,null,2216,"83_15/10/2019 10:34:31 AM","2019-06-10","Defect","Ship Staff","Ship Staff Insp.","Refer.compressor no.2 mech.seal leaking.","E/R - Aux. Mach.,Miscellaneous","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Mech.seal renewed.","2019-06-20",null,"Completed","2019-06-20","No","No","No","Internal"]
[null,null,null,null,2217,"83_15/10/2019 10:35:32 AM","2019-06-11","Defect","Ship Staff","Ship Staff Insp.","5 Nos PV Valve leaking from Vaccum & pressure side.","Inert Gas","Cargo / Ballast Systems","Equipment Related",8.2100000000000009,"High","Not Applicable","Not Applicable","overhauled. Jon completed.","2019-06-26",null,"Completed","2019-06-26","No","No","No","Internal"]
[null,null,null,null,2218,"83_15/10/2019 10:36:43 AM","2019-07-06","Defect","Ship Staff","Ship Staff Insp.","Port Anchor brake cylinder seal leaaking.","Deck - Mooring Machinery","Mooring","Equipment Related",9.1999999999999993,"Medium","Not Applicable","Not Applicable","Seal renewed, leak stopped. Job completed..","2019-07-15",null,"Completed","2019-07-12","No","No","No","Internal"]
[null,null,null,null,2219,"83_15/10/2019 10:38:07 AM","2019-07-11","Defect","Ship Staff","Ship Staff Insp.","Deck seal drain pipe flange leaking in pumproom.\t","Inert Gas","General Appearance","Equipment Related",8.25,"Very High","Not Applicable","Not Applicable","New gasket replaced.","2019-07-15",null,"Completed","2019-07-13","No","No","No","Internal"]
[null,null,null,null,2220,"83_15/10/2019 10:39:08 AM","2019-07-16","Defect","Ship Staff","Ship Staff Insp.","Pipe line from upper pipe duct ( s )to wilden pump for suction found holed.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related",8.8000000000000007,"Medium","Not Applicable","Not Applicable","fabricated & renewed.","2019-07-19",null,"Completed","2019-07-18","No","No","No","Internal"]
[null,null,null,null,2221,"83_15/10/2019 10:40:15 AM","2019-07-27","Defect","Ship Staff","Ship Staff Insp.","STBD PIPE DUCT BILGE ALARM FLOAT FOUND FREEZED.","Deck - Pipe / Fittings","General Appearance","Equipment Related",11.4,"Very High","Not Applicable","Not Applicable"," OVERHAULED. Job completed.","2019-07-29",null,"Completed","2019-07-29","No","No","No","Internal"]
[null,null,null,null,2222,"83_15/10/2019 10:43:30 AM","2019-07-24","Defect","Ship Staff","Ship Staff Insp.","Port Anchor wash valve found leaking.","Deck - Pipe / Fittings","General Appearance","Equipment Related",9.1999999999999993,"Medium","Not Applicable","Not Applicable","Overhauled. Job completed.","2019-08-01",null,"Completed","2019-07-30","No","No","No","Internal"]
[null,null,null,null,2223,"83_15/10/2019 10:45:27 AM","2019-04-13","Defect","Ship Staff","Ship Staff Insp.","Engine room vent fan No 2, impeller blade (1pc) dislodge from hub.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","RO Raised receive in Canaport, Impeller replaced and now working.","2019-07-10","ATHE190027","Completed","2019-07-29","No","No","No","Internal"]
[null,null,null,null,2224,"83_15/10/2019 10:46:49 AM","2019-06-28","Defect","Ship Staff","Ship Staff Insp.","5 % O2 Alarm is not resetting even the O2 is less than 5%.","Inert Gas","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","System checked and O2 sensor wiring to PLC checked, loose connection tighten, now working satisfactory. ","2019-08-30",null,"Completed","2019-07-02","No","No","No","Internal"]
[null,null,null,null,2225,"83_15/10/2019 10:48:01 AM","2019-07-19","Defect","Ship Staff","Ship Staff Insp.","Both Aux Boiler heavily panting during startup and during stoppage.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Work carried out by adjusting supply air of FD fan  and adjusted automizing steam pressure, at the moment both aux boilers are working satisfactory without panting.","2019-07-30",null,"Completed","2019-07-22","No","No","No","Internal"]
[null,null,null,null,2226,"83_15/10/2019 10:49:43 AM","2019-07-28","Defect","Ship Staff","Ship Staff Insp.","No-2 AC Compressor lube oil pump not building pressure, Discharge pressure sensor faulty.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Oil pump and pressure sensor changed with sapre, all satisfactory.","2019-07-30",null,"Completed","2019-07-29","No","No","No","Internal"]
[null,null,null,null,2227,"83_15/10/2019 10:50:45 AM","2019-07-30","Defect","Ship Staff","Ship Staff Insp.","Scrubber tower gas linlet pipline flange gasket blown off.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Gasket renewed, No leak present after testing. All satisfactory.","2019-07-31",null,"Completed","2019-07-30","No","No","No","Internal"]
[null,null,null,null,2228,"83_15/10/2019 10:52:37 AM","2019-07-12","Defect","Ship Staff","Ship Staff Insp.","X band radar scanner's motor carbon brushes worn out.","Critical Equip.","Navigation","Equipment Related",4.3,"Medium","Not Applicable","Not Applicable","Carbon brushes replaced , new spares are on order.","2019-09-30","ATHE190091","Completed","2019-07-12","No","No","No","Internal"]
[null,null,null,null,2229,"83_15/10/2019 10:53:55 AM","2019-07-15","Defect","Ship Staff","Ship Staff Insp.","Hose handling crane starboard two hydraulic hoses defective.","Deck - Machinery","General Appearance","Equipment Related",8.5,"Medium","Not Applicable","Not Applicable","spare hoses replaced with defective hoses.","2019-07-19",null,"Completed","2019-07-16","No","No","No","Internal"]
[null,null,null,null,2230,"83_15/10/2019 10:55:26 AM","2019-07-26","Defect","Ship Staff","Ship Staff Insp.","Rescue boat devit hydraulic motor giving 440V low insulation.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related",10.38,"Medium","Not Applicable","Not Applicable","Motor removed and re varnished and fix back, no 440V insulation alarm is activating after overhaul. ","2019-07-30",null,"Completed","2019-07-29","No","No","No","Internal"]
[null,null,null,null,2231,"83_15/10/2019 10:56:52 AM","2019-08-04","Defect","Ship Staff","Ship Staff Insp.","FWD Winch hydraulic cooling line found holed.","Deck - Machinery","Mooring","Equipment Related",9.1999999999999993,"Medium","Not Applicable","Not Applicable","Fabricated & renewed.","2019-08-06",null,"Completed","2019-08-06","No","No","No","Internal"]
[null,null,null,null,2232,"83_15/10/2019 10:58:03 AM","2019-08-05","Defect","Ship Staff","Ship Staff Insp.","IG to Cargo line found wasted & holed.","Inert Gas","Cargo / Ballast Systems","Equipment Related",11.4,"Very High","Not Applicable","Not Applicable","Fabricated & renewed.","2019-08-15",null,"Completed","2019-08-08","No","No","No","Internal"]
[null,null,null,null,2233,"83_15/10/2019 10:59:14 AM","2019-08-08","Defect","Ship Staff","Ship Staff Insp."," No.1 & No.2 COP AUS discharge valve pneumatic line found leaking.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related",8.11,"Medium","Not Applicable","Not Applicable","Renewed. Job completed.","2019-08-10",null,"Completed","2019-08-09","No","No","No","Internal"]
[null,null,null,null,2234,"83_15/10/2019 11:00:22 AM","2019-08-06","Defect","Ship Staff","Ship Staff Insp.","Fabrication of One section of FWD Winch hydraulic cooling line.","Deck - Mooring Machinery","Mooring","Equipment Related",11.4,"Very High","Not Applicable","Not Applicable","New line fabricated & renewed.","2019-08-15",null,"Completed","2019-08-14","No","No","No","Internal"]
[null,null,null,null,2235,"83_15/10/2019 11:01:40 AM","2019-04-01","Defect","Ship Staff","Ship Staff Insp.","Main Engine Various operational and critical spares need to placed on board eg. ICU, RPME, Crank angle sensor, drain valve etc.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related",10.130000000000001,"Very High","Not Applicable","Not Applicable","Spares ordered and received in full.","2019-07-01","ATHE195022","Completed","2019-07-20","No","No","No","Internal"]
[null,null,null,null,2236,"83_15/10/2019 11:02:52 AM","2019-04-13","Defect","Ship Staff","Suptd. Insp.","Migration to LED Lighting.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","In progress","2019-06-30",null,"Completed","2019-08-20","No","No","No","Internal"]
[null,null,null,null,2237,"83_15/10/2019 11:06:39 AM","2019-08-03","Defect","Ship Staff","Ship Staff Insp.","ME OMD NO 9 SENSOR  FOR  FUEL PUMP GIVING FAULT ALARMS .","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related",10.210000000000001,"Medium","Not Applicable","Not Applicable","REPLACED WITH SPARE NEW ONE  Spare ordered.","2019-09-30","ATHE 190106","Completed","2019-08-20","No","No","No","Internal"]
[null,null,null,null,2238,"83_15/10/2019 11:07:38 AM","2019-08-20","Defect","Ship Staff","Ship Staff Insp.","Fwd winch hydraulic one hydraulic hose found leaking.","Deck - Mooring Machinery","Mooring","Equipment Related",9.14,"Medium","Not Applicable","Not Applicable","Same renewed.","2019-08-25",null,"Completed","2019-08-25","No","No","No","Internal"]
[null,null,null,null,2239,"83_15/10/2019 11:08:44 AM","2019-08-20","Defect","Ship Staff","Ship Staff Insp.","Both LT cooler sea water side are chocked with marine growth, causing LT frersh water temperature to rise.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Both LT cooler sea water side need manual cleaning of plates. Both L.T coolers chemically cleaned all parameters maintaining satisfactory .","2019-09-15",null,"Completed","2019-08-21","No","No","No","Internal"]
[null,null,null,null,2240,"83_15/10/2019 11:10:03 AM","2019-03-26","Defect","Ship Staff","Ship Staff Insp.","Many Pressure gauges faulty in ER need to be replaced.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Supplied at yard and replaced . Will identify more and replace pending in due course.","2019-09-25",null,"Completed","2019-08-15","No","No","No","Internal"]
[null,null,null,null,2241,"83_15/10/2019 11:11:28 AM","2019-04-03","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Soot collecting tank to fabricate for collecting / separating soot.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","To be done in due course of time","2021-07-02",null,"Completed","2019-08-15","No","No","No","Internal"]
[null,null,null,null,2242,"83_15/10/2019 11:12:41 AM","2019-04-13","Defect","Ship Staff","Ship Staff Insp.","ME torsional vibrational damper ( Geslinger ) in ECR not working and alarm active..","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Spare part ordered . Presently the unit is switched off. Will be supplied under next year budget.","2021-07-10","ATHE195071","Completed","2019-08-15","No","No","No","Internal"]
[null,null,null,null,2243,"83_15/10/2019 11:14:08 AM","2019-04-12","Defect","Ship Staff","Ship Staff Insp.","COP No.1 Electric driven system check by makers.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related",8.18,"High","Not Applicable","Not Applicable","Vacon engr to arrange with spares and for further troubleshooting- Technician joined and repaired .","2019-09-05",null,"Completed","2019-08-26","No","No","No","Internal"]
[null,null,null,null,2244,"83_15/10/2019 11:15:26 AM","2019-04-01","Defect","Ship Staff","Ship Staff Insp.","220 volt alarm at many places. Need to replace light bulbs, fititng at many palces.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related",10.38,"Medium","Not Applicable","Not Applicable","Many places rectified in acomodation and lighting and still in progress. Will require to roder light fittings and consumables.","2019-09-30",null,"Completed","2019-08-30","No","No","No","Internal"]
[null,null,null,null,2245,"83_15/10/2019 11:16:30 AM","2019-06-10","Defect","Ship Staff","Ship Staff Insp.","Cargo Pump separator NO.1,2,3 pipe line between Separator & drain line drain line found soft patch.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related",8.8000000000000007,"Medium","Not Applicable","Not Applicable","Temporary repairs carried out.","2019-10-30",null,"Completed","2019-08-15","No","No","No","Internal"]
[null,null,null,null,2246,"83_15/10/2019 11:17:37 AM","2019-08-20","Defect","Ship Staff","Ship Staff Insp.","WECS computer in ECR use for motitoring/ controlling main engine parameters is shutting off (hard drive shutting off) every 15 minutes. ","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Need to replace existing WECS computer CPU with new CPU. - CPU landed at Durban and will receive back , at present original Lap top is in use.","2019-09-15",null,"Completed","2019-08-26","No","No","No","Internal"]
[null,null,null,null,2247,"83_15/10/2019 11:18:48 AM","2019-04-12","Defect","Ship Staff","Ship Staff Insp.","Rail hoses ( inlet ) side not chnaged since new building. Need to replace.\t","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Spares ordered for spare hoses.","2019-09-30",null,"Completed","2019-09-10","No","No","No","Internal"]
[null,null,null,null,2248,"83_15/10/2019 11:20:22 AM","2019-04-12","Defect","Ship Staff","Ship Staff Insp.","Aconis GCE module will require upgrade in due course once starts failing.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Not urgent as presently no issues faced in power management system.","2020-07-10","ATHE195031","Completed","2019-09-10","No","No","No","Internal"]
[null,null,null,null,2249,"83_15/10/2019 11:22:24 AM","2019-04-12","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Himsen DG's will require 2020 modification in due course.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Not urgent and can wait till next year.","2020-07-10",null,"Completed","2019-09-10","No","No","No","Internal"]
[null,null,null,null,2250,"83_15/10/2019 11:24:01 AM","2019-07-26","Defect","Ship Staff","Ship Staff Insp.","No-1 HFO Purifier vertical shaft bearing failed in service.","E/R - Purifier","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Overhaul to carry out.","2019-09-15",null,"Completed","2019-09-10","No","No","No","Internal"]
[null,null,null,null,2251,"83_15/10/2019 11:25:11 AM","2019-09-16","Defect","Ship Staff","Ship Staff Insp.","Control air rubber hose for COP No.2 found leaked during \n\nroutine inspection after departure discharge Sikka, India.\n\n\t","Cargo Mach.","Cargo / Ballast Systems","Equipment Related",8.8000000000000007,"Medium","Not Applicable","Not Applicable","Need to Replace the rubber pipe.","2019-09-30",null,"Completed","2019-09-18","No","No","No","Internal"]
[null,null,null,null,2252,"83_15/10/2019 11:31:31 AM","2019-09-06","Defect","Ship Staff","Ship Staff Insp.","Hydraulic leak found on Port side windlass control lever block .","Deck - Mooring Machinery","Mooring","Equipment Related",9.14,"Medium","Not Applicable","Not Applicable","Rectified.","2019-10-10",null,"Completed","2019-09-07","No","No","No","Internal"]
[null,null,null,null,2253,"83_15/10/2019 11:37:08 AM","2019-08-27","Defect","Ship Staff","Ship Staff Insp.","No:2 DG tacho fail alarm activating during operation.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Faulty speed pick up sensor changed with new spare received at port suez. working satisfactory.","2019-10-15",null,"Completed","2019-10-02","No","No","No","Internal"]
[null,null,null,null,2254,"83_15/10/2019 11:39:29 AM","2019-04-12","Defect","Ship Staff","Ship Staff Insp.","IG vent valve indication glass broken.","Miscellaneous","General Appearance","Equipment Related",8.25,"Very High","Not Applicable","Not Applicable","Replaced with new spare received at port suez.","2019-09-15","ATHE190082","Completed","2019-10-12","No","No","No","Internal"]
[null,null,null,null,2255,"83_15/10/2019 11:41:32 AM","2019-05-21","Defect","Ship Staff","Ship Staff Insp.","E/R signal light coloumns 2 no's in operative.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","PCBs replaced and working fine.","2019-09-30","ATHE190071","Completed","2019-09-27","No","No","No","Internal"]
[null,null,null,null,2256,"83_15/10/2019 11:43:31 AM","2019-07-01","Defect","Ship Staff","Ship Staff Insp.","EVAC system pressure switch defective.\t","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Defective pressure switch replaced with new spare received at port suez.","2019-09-30","ATHE190083","Completed","2019-10-12","No","No","No","Internal"]
[null,null,null,null,2257,"83_15/10/2019 11:45:58 AM","2019-10-07","Defect","Ship Staff","Ship Staff Insp.","Vapour return line STBD side aft main valve actuator found cracked on prior arrival load port checks.","Deck - Pipe / Fittings","General Appearance","Equipment Related",11.4,"Very High","Not Applicable","Not Applicable","Actuator replaced with spare actuator available on board.","2019-10-08",null,"Completed","2019-10-07","No","No","No","Internal"]
[null,null,null,null,2258,"83_17/10/2019 6:37:49 PM","2019-04-01","Defect","Ship Staff","Ship Staff Insp.","Galley oven giving low insulation.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related",10.38,"Medium","Not Applicable","Not Applicable","Spare heating element and thermostat controller receive but it is defective as it gives low insulation.Office has been informed.","2019-09-30","ATHE190115\t","Completed","2019-10-05","No","No","No","Internal"]
[null,null,null,null,2259,"83_17/10/2019 6:39:05 PM","2019-08-20","Defect","Ship Staff","Ship Staff Insp.","MGO chiller sea water side is blocked , chiller to be checked for correct operation.\t","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related",10.31,"Very High","Not Applicable","Not Applicable","Chiller to be checked for correct opertaion, pressure tested.","2019-09-15"," ","Completed","2019-10-10","No","No","No","Internal"]
[null,null,null,null,2260,"83_17/10/2019 6:40:36 PM","2019-10-01","Defect","Ship Staff","Ship Staff Insp.","Galley overboard line developed a pin hole just next to overboard valve, section of pipe need to be replaced.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related",10.31,"Very High","Not Applicable","Not Applicable","Galley overboard pipe section renewed.","2019-10-02",null,"Completed","2019-10-02","No","No","No","Internal"]
[null,null,null,null,2261,"83_17/10/2019 6:41:50 PM","2019-09-22","Defect","Ship Staff","Ship Staff Insp.","Both No-1 and No-2 air condition compressor to repair after Both failed in service.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Vessel received two new aircondition compressor at Suez and both compressor changed to new one. ","2019-10-15",null,"Completed","2019-10-14","No","No","No","Internal"]
[null,null,null,null,8390,"83_Thu Oct 10 2019 20:35:16 GMT+0000 (Coordinated Universal Time)","2019-03-20","Defect","Ship Staff","Ship Staff Insp.","Aconis AMS monitor in ECR console are not original and fitted with normal PC monitor.\t","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Original monitor ordered and fixed","2019-04-30","ATHE195060","Completed","2019-04-24","No","No","No","Internal"]
[null,null,null,null,8391,"83_Sun Nov 10 2019 01:29:21 GMT+0000 (Coordinated Universal Time)","2019-04-10","Defect","Ship Staff","Ship Staff Insp.","Steering gear No 1 pp having oil leak from pp block. Need to check leak location.\t\t","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Pump casing block tightened and found no leak on the pump side.","2019-04-30",null,"Completed","2019-04-24","No","No","No","Internal"]
[null,null,null,null,8392,"83_Fri Oct 11 2019 01:33:07 GMT+0000 (Coordinated Universal Time)","2019-04-09","Defect","Ship Staff","Ship Staff Insp.","ME fuel oil fine filter change over mechanism hard.\t","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Change over mechanism overhauled and now its working satisfactory.","2019-04-15",null,"Completed","2019-04-10","No","No","No","Internal"]
[null,null,null,null,8393,"83_Sun Nov 10 2019 01:36:16 GMT+0000 (Coordinated Universal Time)","2019-03-30","Defect","Ship Staff","Ship Staff Insp.","Dust in many electric panels. Many contacts causing low insulation alarm. To clean them and order spares contacts.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related",10.38,"Medium","Not Applicable","Not Applicable","MSBD and AMS panel cleaning carried out at yard. Spare contactors ordered.","2019-04-10","ATHE195030","Completed","2019-04-04","No","No","No","Internal"]
[null,null,null,null,8394,"83_Sun Nov 10 2019 01:38:36 GMT+0000 (Coordinated Universal Time)","2019-04-12","Defect","Ship Staff","Ship Staff Insp.","IG panel turn switch malfuntion. Presently wire disconnected.","Inert Gas","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Switch repaired and its function check carried out.","2019-04-15",null,"Completed","2019-04-14","No","No","No","Internal"]
[null,null,null,null,8395,"83_Sun Nov 10 2019 01:41:57 GMT+0000 (Coordinated Universal Time)","2019-04-02","Defect","Ship Staff","Ship Staff Insp.","Residual BN and Iron to measure and OBSERVE the liner surface. LO test kit to order.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related",10.7,"Medium","Not Applicable","Not Applicable","Test kit received and samples send for shore analysis. Onboard test to be carried out shortly.","2019-04-29",null,"Completed","2019-04-29","No","No","No","Internal"]
[null,null,null,null,8396,"83_Sun Nov 10 2019 01:46:10 GMT+0000 (Coordinated Universal Time)","2019-03-30","Defect","Ship Staff","Ship Staff Insp.","Hydraulic top bracing FWD leaking when charging oil. Suspect cylinder seal damaged and require replacement.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Gas changed in accumulator. As off now no leak is observed and have 1set of seals as spares.","2019-05-30",null,"Completed","2019-04-25","No","No","No","Internal"]
[null,null,null,null,8397,"83_Sun Nov 10 2019 01:49:41 GMT+0000 (Coordinated Universal Time)","2019-04-12","Defect","Ship Staff","Ship Staff Insp.","ME lub oil sump to top up with 6000 litres of oil as presently level around 36,000 ltr.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Sump oil topped up with 6500 litres.","2019-04-15",null,"Completed","2019-04-13","No","No","No","Internal"]
[null,null,null,null,8398,"83_Sun Nov 10 2019 01:51:39 GMT+0000 (Coordinated Universal Time)","2019-03-30","Defect","Ship Staff","Ship Staff Insp.","DG No.3 exhaust gas temp A sensor to be replaced.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Sensor replaced with spare new sensor.","2019-04-25",null,"Completed","2019-04-25","No","No","No","Internal"]
[null,null,null,null,8399,"83_Sun Nov 10 2019 01:54:46 GMT+0000 (Coordinated Universal Time)","2019-04-08","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","No recovery unit / pump - bottles for Main ac for collecting gas.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Received at call singapore","2019-04-25",null,"Completed","2019-04-23","No","No","No","Internal"]
[null,null,null,null,8400,"83_Sun Nov 10 2019 01:56:41 GMT+0000 (Coordinated Universal Time)","2019-03-17","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","WECS computer for wartisila need to upgrade.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Upgraded with new software and hardware.","2019-04-25",null,"Completed","2019-04-23","No","No","No","Internal"]
[null,null,null,null,8401,"83_Sun Nov 10 2019 01:58:31 GMT+0000 (Coordinated Universal Time)","2019-03-21","Defect","Ship Staff","Ship Staff Insp.","Engine performance system for AE and ME","E/R - Aux. Engine,E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","ME and DG performance taken.","2019-04-26",null,"Completed","2019-04-26","No","No","No","Internal"]
[null,null,null,null,8402,"83_Sun Nov 10 2019 14:49:52 GMT+0000 (Coordinated Universal Time)","2019-04-05","Defect","Ship Staff","Ship Staff Insp.","Damaged and Oil soaked lagging to be replaced in some loacations in the Engine room.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related",10.19,"Very High","Not Applicable","Not Applicable","All damaged laggings replaced with spare laggings.","2019-04-25",null,"Completed","2019-04-25","No","No","No","Internal"]
[null,null,null,null,8403,"83_Sun Nov 10 2019 14:52:04 GMT+0000 (Coordinated Universal Time)","2019-03-28","Defect","Ship Staff","Ship Staff Insp.","IG additional O2 panel installation ( MESQAC requirement)","Inert Gas","Eng. / Strg. Comp.","Equipment Related",8.2200000000000006,"Very High","Not Applicable","Not Applicable","New O2 panel installed with all the fittings.","2019-04-25",null,"Completed","2019-04-18","No","No","No","Internal"]
[null,null,null,null,8404,"83_Sun Nov 10 2019 14:54:31 GMT+0000 (Coordinated Universal Time)","2019-04-03","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Boiler and Composite boilers need service engineers to check the settings for IG and water level controllers.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Kangrim service Engineers attended at singapore. Both Aux. boilers are operating satisfactory.","2019-04-25",null,"Completed","2019-04-22","No","No","No","Internal"]
[null,null,null,null,8405,"83_Sun Nov 10 2019 14:56:41 GMT+0000 (Coordinated Universal Time)","2019-04-07","Defect","Ship Staff","Ship Staff Insp.","Emergency generator cooling water pressure switch bypassed.","Elect. Mach. & Equip.","Emgcy. Systems","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Pressure switch renewed.","2019-04-25",null,"Completed","2019-04-24","No","No","No","Internal"]
[null,null,null,null,8406,"83_Sun Nov 10 2019 15:02:49 GMT+0000 (Coordinated Universal Time)","2019-04-05","Defect","Ship Staff","Ship Staff Insp.","Hot water calorifier steam heater body gasket leaking.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Gasket renewed. No leaks in the system.","2019-04-10",null,"Completed","2019-04-05","No","No","No","Internal"]
[null,null,null,null,8407,"83_Fri Oct 11 2019 15:05:18 GMT+0000 (Coordinated Universal Time)","2019-04-02","Defect","Ship Staff","Ship Staff Insp.","Blue line bulkhead master valve suspect passing.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related",8.11,"Medium","Not Applicable","Not Applicable","RO received, Job completed.","2019-04-15","ATHE195057","Completed","2019-04-12","No","No","No","Internal"]
[null,null,null,null,8408,"83_Sun Nov 10 2019 15:12:40 GMT+0000 (Coordinated Universal Time)","2019-04-10","Defect","Ship Staff","Ship Staff Insp.","440 Volt alarm due to low insulation from ER vent fan and Boiler no:1 panel. Need investigation.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related",10.38,"Medium","Not Applicable","Not Applicable","Boiler No:1 faulty contactor replaced and ER vent fan naked wire insulated. 440V insulation meter shows now infinity.","2019-04-13",null,"Completed","2019-04-11","No","No","No","Internal"]
[null,null,null,null,8409,"83_Sun Nov 10 2019 15:15:09 GMT+0000 (Coordinated Universal Time)","2019-04-22","Defect","Ship Staff","Ship Staff Insp.","Emergency fire pump not building pressure.","Critical Equip.","Eng. / Strg. Comp.","Equipment Related",5.41,"Very High","Not Applicable","Not Applicable","Priming pump engaging lever found broken, same welded. Pump tried out and found to be woeking satisfactory.","2019-04-23",null,"Completed","2019-04-23","No","No","No","Internal"]
[null,null,null,null,8410,"83_Fri Oct 11 2019 15:27:32 GMT+0000 (Coordinated Universal Time)","2019-04-22","Defect","Ship Staff","Ship Staff Insp.","OWS 3-way valve malfunctioning on test mode.","Critical Equip.","Eng. / Strg. Comp.","Equipment Related",6.17,"Very High","Not Applicable","Not Applicable","Complete unit replaced by the shore w/shop UNI Marine services Singapore ( Cell + Calib.unit). Tried out and found to be working.","2019-04-23",null,"Completed","2019-04-23","No","No","No","Internal"]
[null,null,null,null,8411,"83_Sun Nov 10 2019 15:38:20 GMT+0000 (Coordinated Universal Time)","2019-04-24","Defect","Ship Staff","Ship Staff Insp.","Bilge pump not taking suc.properly.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related",6.14,"High","Not Applicable","Not Applicable","Assy.dismantled. Valve and valve seat having piting marks , same build up by steel putty and lapped. Pump tried out-working ok.","2019-04-24",null,"Completed","2019-04-24","No","No","No","Internal"]
[null,null,null,null,8412,"83_Tue Dec 10 2019 03:44:30 GMT+0000 (Coordinated Universal Time)","2019-03-08","Defect","Ship Staff","Ship Staff Insp.","OWS ist stage filter fully wasted/oil soaked","Critical Equip.","Eng. / Strg. Comp.","Equipment Related",6.17,"Very High","Not Applicable","Not Applicable","First stage filter replaced with the spare one.","2019-04-30",null,"Completed","2019-04-24","No","No","No","Internal"]
[null,null,null,null,8413,"83_Tue Dec 10 2019 03:46:20 GMT+0000 (Coordinated Universal Time)","2019-03-20","Defect","Ship Staff","Ship Staff Insp.","Fire bilge and GS pump No.1 Mechanical seal leaking.","LSA / FFA","Eng. / Strg. Comp.","Equipment Related",5.38,"High","Not Applicable","Not Applicable","Mech.seal replaced with the spare one.","2019-04-30",null,"Completed","2019-04-25","No","No","No","Internal"]
[null,null,null,null,8414,"83_Sat Oct 12 2019 03:47:47 GMT+0000 (Coordinated Universal Time)","2019-04-25","Defect","Ship Staff","Ship Staff Insp.","Air.cond.compressor no.2 mech.seal leaking.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Mech.seal replaced with the spare one.","2019-04-27",null,"Completed","2019-04-25","No","No","No","Internal"]
[null,null,null,null,8415,"83_Tue Dec 10 2019 03:49:10 GMT+0000 (Coordinated Universal Time)","2019-04-12","Defect","Ship Staff","Ship Staff Insp.","DG 2 fuel filter leaking oil from top.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related",10.19,"Very High","Not Applicable","Not Applicable","Leakage rectified.","2019-04-30",null,"Completed","2019-04-26","No","No","No","Internal"]
[null,null,null,null,8416,"83_Tue Dec 10 2019 03:52:13 GMT+0000 (Coordinated Universal Time)","2019-03-30","Defect","Ship Staff","Ship Staff Insp.","IG scrubber high level float alarm erratic and temporarily repaired.","Inert Gas","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","High level float renewed and tried out-satisfactory.","2019-04-30",null,"Completed","2019-04-26","No","No","No","Internal"]
[null,null,null,null,8417,"83_Tue Dec 10 2019 03:53:58 GMT+0000 (Coordinated Universal Time)","2019-04-05","Defect","Ship Staff","Ship Staff Insp.","Incinerator refractory to order. Sludge burning to start in incinrateor.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Refractory is in good condition. Sludge burning started in incinerator.","2019-04-28",null,"Completed","2019-04-26","No","No","No","Internal"]
[null,null,null,null,8418,"83_Tue Dec 10 2019 03:55:40 GMT+0000 (Coordinated Universal Time)","2019-03-20","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Graviner oil mist detector EPROM and software upgrade.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related",10.210000000000001,"Medium","Not Applicable","Not Applicable","monitoring and no issues till now. ","2019-05-30",null,"Completed","2019-04-26","No","No","No","Internal"]
[null,null,null,null,8419,"83_Tue Dec 10 2019 03:58:05 GMT+0000 (Coordinated Universal Time)","2019-04-12","Defect","Ship Staff","Ship Staff Insp.","Inert gas temp found to be going higher withing short period of operation.","Inert Gas","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Scruuber tower all nozzles removed and cleared off dirt/sea shells.","2019-05-30",null,"Completed","2019-04-26","No","No","No","Internal"]
[null,null,null,null,8420,"83_Sat Oct 12 2019 04:00:27 GMT+0000 (Coordinated Universal Time)","2019-04-02","Defect","Ship Staff","Ship Staff Insp.","4C COT Stripper valve passing.","Deck - Machinery","Cargo / Ballast Systems","Equipment Related",8.11,"Medium","Not Applicable","Not Applicable","Seat ring  renewed","2019-04-16","ATHE195057","Completed","2019-04-16","No","No","No","Internal"]
[null,null,null,null,8421,"83_Tue Dec 10 2019 05:02:49 GMT+0000 (Coordinated Universal Time)","2019-04-12","Defect","Ship Staff","Ship Staff Insp.","Kongsberg System Max. depths for all centre tanks needs to be corrected  noted a difference in the Max. depths in the sounding tables and the actual on board.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related",8.1199999999999992,"Medium","Not Applicable","Not Applicable","Kongberg technician needed to attend the same // SERVICE ENGR ATTENDED AT SINGAPORE ON 22 APR. FAULT RECTIFIED.","2019-04-22",null,"Completed","2019-04-22","No","No","No","Internal"]
[null,null,null,null,8422,"83_Tue Dec 10 2019 05:09:10 GMT+0000 (Coordinated Universal Time)","2019-04-12","Defect","Ship Staff","Ship Staff Insp.","Ballast Sea chest Valve cannot be opened from the Cargo Control Room. Need to open / shut using hand pump.","Deck - Machinery","Eng. / Strg. Comp.","Equipment Related",8.11,"Medium","Not Applicable","Not Applicable","Technician in singapore attended // FAULT RECTIFIED.","2019-04-22",null,"Completed","2019-04-22","No","No","No","Internal"]
[null,null,null,null,8423,"83_Tue Dec 10 2019 06:14:42 GMT+0000 (Coordinated Universal Time)","2019-04-02","Defect","Ship Staff","Ship Staff Insp.","Cargo and Bunker Overfill alarm hooters on deck not working. ","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related",8.14,"Very High","Not Applicable","Not Applicable","RO Raised, spares received at Canaport, deck overfill alarm hooters working, bunker overfill alarm hooter remains ATHE190089.","2019-04-22","ATHE190033 & ATHE190089","Completed","2019-04-22","No","No","No","Internal"]
[null,null,null,null,8424,"83_Tue Dec 10 2019 06:17:20 GMT+0000 (Coordinated Universal Time)","2019-04-02","Defect","Ship Staff","Ship Staff Insp.","Both pilot ladders not solas approved.\t\t","LSA / FFA","LSA / FFA Appliances","Equipment Related",5.47,"Medium","Not Applicable","Not Applicable","RO RECEIVED,  NEW PILOT LADDER  RECEIVED & IN USE.","2019-04-22","ATHE195079","Completed","2019-04-22","No","No","No","Internal"]
[null,null,null,null,8425,"83_Tue Dec 10 2019 06:19:04 GMT+0000 (Coordinated Universal Time)","2019-04-02","Defect","Ship Staff","Ship Staff Insp.","6 Nos Mandal shackle need renewal, Found wasted.","Deck - Machinery","General Appearance","Equipment Related",9.17,"High","Not Applicable","Not Applicable","NEW MANDAL SHACKLE RECEIVED & RENEWED.","2019-04-22","ATHE190031","Completed","2019-04-22","No","No","No","Internal"]
[null,null,null,null,8426,"83_Tue Dec 10 2019 06:26:08 GMT+0000 (Coordinated Universal Time)","2019-04-12","Defect","Ship Staff","Ship Staff Insp.","NO.2 BALLAST PUMP DISCHARGE PRESSURE TRANSMITTER SHOWING PRESSURE BUT ACTUAL ITS ZERO","Elect. Mach. & Equip.","Cargo / Ballast Systems","Equipment Related",8.8000000000000007,"Medium","Not Applicable","Not Applicable","Pressure transmitter changed, working satisfactory.","2019-04-19",null,"Completed","2019-04-19","No","No","No","Internal"]
[null,null,null,null,8427,"83_Tue Dec 10 2019 06:29:24 GMT+0000 (Coordinated Universal Time)","2019-04-12","Defect","Ship Staff","Ship Staff Insp.","Cargo seachest valve not fitted with regulator.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related",8.11,"Medium","Not Applicable","Not Applicable","REGULATOR RECEIVED & RENEWED.","2019-04-22","ATHE195090","Completed","2019-04-22","No","No","No","Internal"]
[null,null,null,null,8428,"83_Tue Dec 10 2019 06:31:34 GMT+0000 (Coordinated Universal Time)","2019-04-12","Defect","Ship Staff","Ship Staff Insp.","1S COT Overfill alarm float stuck.\t","Elect. Mach. & Equip.","Cargo / Ballast Systems","Equipment Related",8.14,"Very High","Not Applicable","Not Applicable","overhauled & Working satisfactory after overhaul. ","2019-04-16",null,"Completed","2019-04-16","No","No","No","Internal"]
[null,null,null,null,8429,"83_Tue Dec 10 2019 06:32:58 GMT+0000 (Coordinated Universal Time)","2019-04-12","Defect","Ship Staff","Ship Staff Insp.","Cargo, Ballast, Pumproom valves indicators showing erratic.\t","Elect. Mach. & Equip.","Cargo / Ballast Systems","Equipment Related",8.11,"Medium","Not Applicable","Not Applicable","overhauled & Working satisfactory after overhaul. ","2019-04-23",null,"Completed","2019-04-23","No","No","No","Internal"]
[null,null,null,null,8430,"83_Tue Dec 10 2019 06:32:24 GMT+0000 (Coordinated Universal Time)","2019-04-02","Defect","Ship Staff","Ship Staff Insp.","Slop s COT Valve passing.","Deck - Machinery","Cargo / Ballast Systems","Equipment Related",8.11,"Medium","Not Applicable","Not Applicable","Seat ring renewed.","2019-04-28","ATHE195057","Completed","2019-04-30","No","No","No","Internal"]
[null,null,null,null,8431,"83_Sat Oct 12 2019 06:33:47 GMT+0000 (Coordinated Universal Time)","2019-04-22","Defect","Ship Staff","Ship Staff Insp.","Oil traces found in the observation tank.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Main engine fuel oil heater no.2 found 1no tube leaking,same plugged.Again pr.tested and observed no leaks.We will keep monitoring.","2019-05-30",null,"Completed","2019-05-02","No","No","No","Internal"]
[null,null,null,null,8432,"83_Tue Dec 10 2019 06:35:56 GMT+0000 (Coordinated Universal Time)","2019-05-01","Defect","Ship Staff","Ship Staff Insp.","FWG dosing pump non functional.","E/R - Aux. Mach.","Emgcy. Systems","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Pump dismantled ,inspected and all parts cleaned.Discharge line found clogged,same cleared.","2019-05-10",null,"Completed","2019-05-03","No","No","No","Internal"]
[null,null,null,null,8433,"83_Tue Dec 10 2019 06:37:40 GMT+0000 (Coordinated Universal Time)","2019-05-01","Defect","Ship Staff","Ship Staff Insp.","Main engine booster pump no.2 not building sufficient pressure.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Fault traced with the relief valve.Same dismantled, o'hauled and relief v/v adjusted.","2019-05-12",null,"Completed","2019-05-04","No","No","No","Internal"]
[null,null,null,null,8434,"83_Tue Dec 10 2019 06:39:06 GMT+0000 (Coordinated Universal Time)","2019-04-02","Defect","Ship Staff","Ship Staff Insp.","VECS System pressure guage not working in CCR.","Elect. Mach. & Equip.","Emgcy. Systems","Equipment Related",8.25,"Very High","Not Applicable","Not Applicable","This was due to wrong connections given in shipyard,same rectified.","2019-05-10",null,"Completed","2019-05-07","No","No","No","Internal"]
[null,null,null,null,8435,"83_Tue Dec 10 2019 06:40:59 GMT+0000 (Coordinated Universal Time)","2019-04-21","Defect","Ship Staff","Ship Staff Insp.","Stbd Windlass Brake Cylinder leaking.","Deck - Mooring Machinery","Mooring","Equipment Related",9.1999999999999993,"Medium","Not Applicable","Not Applicable","Seals renewed.Brake cyl.tested and observed no leaks .","2019-05-05",null,"Completed","2019-05-07","No","No","No","Internal"]
[null,null,null,null,8436,"83_Tue Dec 10 2019 06:42:22 GMT+0000 (Coordinated Universal Time)","2019-04-12","Defect","Ship Staff","Ship Staff Insp.","7 Nos. Foam Monitor valves leaking. ","LSA / FFA","General Appearance","Equipment Related",5.38,"High","Not Applicable","Not Applicable","Valves renewed.","2019-05-06","ATHE190037","Completed","2019-05-09","No","No","No","Internal"]
[null,null,null,null,8437,"83_Tue Dec 10 2019 06:44:50 GMT+0000 (Coordinated Universal Time)","2019-04-02","Defect","Ship Staff","Ship Staff Insp.","2P WBT Main valve passing.","Deck - Pipe / Fittings","General Appearance","Equipment Related",8.11,"Medium","Not Applicable","Not Applicable","Valve seat ring renewed.","2019-05-13",null,"Completed","2019-05-11","No","No","No","Internal"]
[null,null,null,null,8438,"83_Tue Dec 10 2019 06:46:34 GMT+0000 (Coordinated Universal Time)","2019-05-06","Defect","Ship Staff","Ship Staff Insp.","Hydraulic leak in MW6 Winch remote opeartion pressure line .","Deck - Mooring Machinery","Mooring","Equipment Related",9.14,"Medium","Not Applicable","Not Applicable","Leakage rectified.","2019-05-13",null,"Completed","2019-05-14","No","No","No","Internal"]
[null,null,null,null,8439,"83_Tue Dec 10 2019 06:48:52 GMT+0000 (Coordinated Universal Time)","2019-04-10","Defect","Ship Staff","Ship Staff Insp.","Stbd windlass Hyd cylinder for engaing / disengaging gear is not working.","Deck - Mooring Machinery","Mooring","Equipment Related",9.1999999999999993,"Medium","Not Applicable","Not Applicable","Hyd.cylinder eased up and found to working satisfactory.","2019-07-08",null,"Completed","2019-05-14","No","No","No","Internal"]
[null,null,null,null,8440,"83_Tue Dec 10 2019 06:50:29 GMT+0000 (Coordinated Universal Time)","2019-05-14","Defect","Ship Staff","Ship Staff Insp.","Hydraulic leak in MW2 Winch remote opeartion pressure line.","Deck - Mooring Machinery","Mooring","Equipment Related",9.14,"Medium","Not Applicable","Not Applicable","Leakage rectified.","2019-05-16",null,"Completed","2019-05-15","No","No","No","Internal"]
[null,null,null,null,8441,"83_Tue Dec 10 2019 06:53:02 GMT+0000 (Coordinated Universal Time)","2019-04-23","Defect","Ship Staff","Ship Staff Insp.","No.2 Ballast pump suction guage found inoperational.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related",8.8000000000000007,"Medium","Not Applicable","Not Applicable","Suction gauge repaired  & Working satisfactory after overhaul. ","2019-05-14",null,"Completed","2019-05-15","No","No","No","Internal"]
[null,null,null,null,8442,"83_Tue Dec 10 2019 06:54:46 GMT+0000 (Coordinated Universal Time)","2019-05-16","Defect","Ship Staff","Ship Staff Insp.","Composite boiler feed water pump no.2 mech.seal leaking.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related",10.31,"Very High","Not Applicable","Not Applicable","Pump and motor o'hauled.Tried out-all in order.","2019-05-17",null,"Completed","2019-05-16","No","No","No","Internal"]
[null,null,null,null,8443,"83_Tue Dec 10 2019 06:56:04 GMT+0000 (Coordinated Universal Time)","2019-05-16","Defect","Ship Staff","Ship Staff Insp.","DGs fuel oil heater no.2 relief valve leaking.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Relief valve dismantled,inspected and all parts cleaned.Heater put back in use and found no leaks.","2019-05-20",null,"Completed","2019-05-18","No","No","No","Internal"]
[null,null,null,null,8444,"83_Tue Dec 10 2019 06:57:18 GMT+0000 (Coordinated Universal Time)","2019-04-02","Defect","Ship Staff","Ship Staff Insp.","SEVERAL WHEELS FOR COW MACHINE VALVE & FIRE LINE FOUND BROKEN & DAMAGED.\t\t","Cargo Mach.","Cargo / Ballast Systems","Equipment Related",8.8000000000000007,"Medium","Not Applicable","Not Applicable","All renewed","2019-05-20",null,"Completed","2019-05-18","No","No","No","Internal"]
[null,null,null,null,8445,"83_15/12/2019 2:35:21 AM","2019-09-12","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Steering gear room hydraulic oil drums was arranged with direct contact with the floor plate. ","Miscellaneous","Eng. / Strg. Comp.","Inappropriate Procedure",10.29,"Medium","Not Applicable","Not Applicable","Steering gear room hydraulic oil drums was arranged with a wooden pallets at the base.","2019-09-30",null,"Completed","2019-11-04","No","No","No","Internal"]
[null,null,null,null,8446,"83_Mon Mar 11 2019 01:33:01 GMT+0000 (Coordinated Universal Time)","2019-10-29","Defect","Ship Staff","Ship Staff Insp.","Aux.Boiler No: 1 - Found Top Manhole gasket leaking when boiler is pressurized","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Boiler to be de-pressurized and Manhole gasket renewed.","2019-11-15",null,"Completed","2019-11-06","No","No","No","Internal"]
[null,null,null,null,8447,"83_15/12/2019 2:43:00 AM","2019-11-05","Defect","Ship Staff","Ship Staff Insp.","No : 1 AC Compressor Pin hole on compressor HP discharge valve line.Hot work to be carried out.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","No : 1 AC Compressor isolated , gas collected in recovery bottled and  Pin hole on compressor HP discharge valve line brazed. Hot work permission obtained from office for the same and Hot work permit  made.","2019-11-30",null,"Completed","2019-11-15","No","No","No","Internal"]
[null,null,null,null,8448,"83_15/12/2019 2:50:31 AM","2019-11-30","Defect","Ship Staff","Ship Staff Insp.","Main Steam stop valve (line valve) of  #1 and #2 boilers - Bonnet gasket leaking","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Main Steam stop valve (line valve) of  #1 and #2 boilers - Bonnet gaskets renewed. Boilers depressurized valve bonnet opened and gasket renewed.","2019-12-06",null,"Completed","2019-12-04","No","No","No","Internal"]
[null,null,null,null,8449,"83_15/12/2019 3:00:53 AM","2019-10-28","Defect","Ship Staff","Ship Staff Insp.","Main Engine F.O Booster pump No 2 - Found making abnormal noise. Pump to be opened up and checked. ","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Re-Conditioned pump complete (with motor) was receieved at Kwinana port. Same was installed and pump tried out.Found satisfactory.","2019-12-15",null,"Completed","2019-12-14","No","No","No","Internal"]
[null,null,null,null,8450,"83_Mon Mar 11 2019 01:25:37 GMT+0000 (Coordinated Universal Time)","2019-10-26","Defect","Ship Staff","Ship Staff Insp.","Foam Station Telephone - found not working /operational","Elect. Mach. & Equip.","Communication","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Faulty mic replaced with spare one. tried out working fine.","2019-11-15",null,"Completed","2019-12-01","No","No","No","Internal"]
[null,null,null,null,8451,"83_15/12/2019 3:32:35 AM","2019-12-01","Defect","Ship Staff","Ship Staff Insp.","Main Engine - Fuel Pump #2 Actuator is found sluggish. To be opened up and carbon brushes renewed. ","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Actuator carbon brushes received at Kwinana port.Same was used and Fuel pump # 2 Actuator overhauled. Engine tried out and found satisfactory.","2019-12-15",null,"Completed","2019-12-12","No","No","No","Internal"]
[null,null,null,null,8452,"83_15/12/2019 3:37:07 AM","2019-12-13","Defect","Ship Staff","Ship Staff Insp.","Main Engine L.O pump # 2 - MCCB was found tripping while starting. Problem to be investigated.\t","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Found timer for Y-D change over timer faulty. Same renewed with spare one. pump tried out found working satisfactory.","2019-12-14",null,"Completed","2019-12-14","No","No","No","Internal"]
[null,null,null,null,8453,"83_15/12/2019 3:42:21 AM","2019-11-14","Defect","Ship Staff","Ship Staff Insp.","Elevator found door controller PCB defective. Door was found not opening and close limit switch LED was seen continuously  ON even when door was open. ","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Replaced PCB with spare received at Kwinana. PCB calibrated and elevator tried out. Found satisfactory. ","2019-12-15",null,"Completed","2019-12-12","No","No","No","Internal"]
[null,null,null,null,8791,"83_Fri Dec 20 2019 18:37:11 GMT+0000 (Coordinated Universal Time)","2019-12-10","Defect","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","Rescue boat davit operation on stored hydraulic power was very slow & sluggish.","LSA / FFA","LSA / FFA Appliances","Equipment Related",5.29,"High","Not Applicable","Not Applicable","Shore technician from denray Marine attendenance onboard on 14 Dec 2019 at Outer Anchorage, Fremantle, Western Australia after completion of first STS. Rescue boat davit found to be working good after shore servicing.","2020-01-10",null,"Completed","2019-12-14","No","No","No","External"]
[null,null,null,null,8792,"83_Fri Dec 20 2019 18:41:44 GMT+0000 (Coordinated Universal Time)","2019-12-10","Defect","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","Emergency light for rescue boat & one emergency light for the free fall life boat were not working. same was repaired before the end of inspection.","Elect. Mach. & Equip.","Emgcy. Systems","Equipment Related",11.9,null,"Not Applicable","Not Applicable","Rectified before completion of inspection.","2019-12-11",null,"Completed","2019-12-10","No","No","No","External"]
[null,null,null,null,null,"83_17/10/2019 6:07:21 PM","2019-06-13","Defect","Ship Staff","Ship Staff Insp.","PV Breaker drain line found pin hole.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related",8.2799999999999994,"Medium","Not Applicable","Not Applicable","Temporary repairs carried out. - 17/06/19\t","2019-10-30"," ","Completed","2019-10-30","No",null,null,"Internal"]
[null,null,null,null,null,"83_17/10/2019 6:04:36 PM","2019-05-15","Defect","Ship Staff","Ship Staff Insp.","Draft readings not showing correct in K Guage Tank Radar system display in CCR.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related",8.8000000000000007,"Medium","Not Applicable","Not Applicable","Technician need to attend ,Recaliberate .","2019-11-30"," ","Completed","2019-11-30","No",null,null,"Internal"]
[null,null,null,null,null,"83_16/10/2019 6:28:39 PM","2019-04-12","Defect","Ship Staff","Ship Staff Insp.","Ballast remote sounding guages for all tanks showing erratic readings except 1P ","Cargo Mach.","Cargo / Ballast Systems","Equipment Related",8.8000000000000007,"Medium","Not Applicable","Not Applicable","Ballast tanks purge heads dismantled, overhauled,cleaned & cleared. Two purge unit  requisitioned raised. Will check the trueness of readings  during discharging opeartion.","2019-11-15","ATHE195089\t","Completed","2019-12-30","No",null,null,"Internal"]
[null,null,null,null,null,"83_17/10/2019 6:26:14 PM","2019-09-07","Defect","Ship Staff","Ship Staff Insp.","STBD anchor wash pipe leaking, found pin hole.","Deck - Pipe / Fittings","General Appearance","Equipment Related",11.4,"Very High","Not Applicable","Not Applicable","Need to fabricate & Renew.","2019-11-10"," ","Completed","2019-11-10","No",null,null,"Internal"]
[null,null,null,null,null,"83_17/10/2019 6:29:07 PM","2019-10-07","Defect","Ship Staff","Ship Staff Insp.","Vapour return line stbd side aft drain valve found cracked on Prior arrival load port checks.","Deck - Pipe / Fittings","General Appearance","Equipment Related",8.25,"Very High","Not Applicable","Not Applicable","Temporary repair carried out.","2019-11-15"," ","Completed","2019-11-15","No",null,null,"Internal"]
[null,null,null,null,null,"83_17/10/2019 6:08:53 PM","2019-06-28","Defect","Ship Staff","Ship Staff Insp.","No.1 Copt suc.pressure transmitter defective.","Cargo Mach.","Eng. / Strg. Comp.","Equipment Related",8.8000000000000007,"Medium","Not Applicable","Not Applicable","Spares needed to replace existing defective pressure transmitter. ","2019-09-15","ATHE190110\t","Completed","2019-11-24","No",null,null,"Internal"]
[null,null,null,null,null,"83_17/10/2019 6:20:33 PM","2019-08-24","Defect","Ship Staff","Ship Staff Insp.","In No.2C Upper stool space located between 2C COT & 3C COT, Minor leak observed on F&A Bulkhead of 2C COT Aft entrance hatch enclosure, just forward of Frame 88 and below 2nd Transverse Bulkhead stiffner support from top.","Hull & Tanks","Structural Condn. / WT integrity ","Equipment Related",8.8000000000000007,"Medium","Not Applicable","Not Applicable","Temporary repairs carried out ON 27/08/19.","2019-12-31"," ","Completed","2019-11-21","No",null,null,"Internal"]
[null,null,null,null,null,"83_17/10/2019 6:21:50 PM","2019-08-24","Defect","Ship Staff","Ship Staff Insp.","\tIn No.2Stbd. Upper stool space located between 2C COT & 3C COT, Minor leak observed on F&A Bulkhead of 3C COT Fwd entrance hatch enclosure, just forward of Frame 88 and below 3rd   Transverse Bulkhead stiffner support from top. ","Hull & Tanks","Structural Condn. / WT integrity ","Equipment Related",8.8000000000000007,"Medium","Not Applicable","Not Applicable","Temporary repairs carried out ON 27/08/19.","2019-12-31"," ","Completed","2019-11-22","No",null,null,"Internal"]
[null,null,null,null,null,"83_17/10/2019 6:23:07 PM","2019-08-27","Defect","Ship Staff","Ship Staff Insp.","In No.4C Upper stool space located between 4C COT & 5C COT, 3 Minor leak observed on F&A Bulkhead of 4C COT Aft entrance hatch enclosure, just forward of Frame 70 and below 1ST,2nd & 3RD Transverse Bulkhead stiffner support from top.","Hull & Tanks","Structural Condn. / WT integrity ","Equipment Related",8.8000000000000007,"Medium","Not Applicable","Not Applicable","Temporary repairs carried out on 02/09/19.","2019-12-31"," ","Completed","2019-11-24","No",null,null,"Internal"]
[null,null,null,null,null,"83_17/10/2019 6:27:38 PM","2019-09-06","Defect","Ship Staff","Ship Staff Insp.","Mastriser valve ( 650 A ) opearting wheel turning freely, Suspect seat ring damage or locking pin of disc damaged .","Cargo Mach.","Cargo / Ballast Systems","Equipment Related",8.25,"Very High","Not Applicable","Not Applicable","Mast Riser Valve removed from place and found Seat Ring damaged. IG 41 V/V (IG to Ballast line) removed and fitted in place of Mast Riser valve. Awaiting spare seat ring for leaking IG Mast Riser Valve.","2019-11-10"," ","Completed","2019-10-07","No",null,null,"Internal"]
[null,null,null,null,null,"83_21/12/2019 8:45:18 AM","2019-12-10","Defect","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","Officer's smoking room exhaust stencil found faded.","Miscellaneous","General Appearance","Inappropriate Procedure",5.0999999999999996,"High","Not Applicable","Not Applicable","TO re stencil the space.","2019-12-31",null,"Completed","2019-12-27","No",null,null,"External"]
[null,null,null,null,null,"83_25/12/2019 9:46:10 AM","2019-12-23","Defect","Ship Staff","Ship Staff Insp.","Lashing ropes for bunker valves on port manifold is missing.","Miscellaneous","Cargo / Ballast Systems","Industry Issue",8.11,"Medium","Not Applicable","Not Applicable","To fix new lashing ropes for the missing one.","2019-12-31",null,"Completed","2019-12-29","No",null,null,"Internal"]
[null,null,null,null,null,"83_21/12/2019 8:41:29 AM","2019-12-10","Defect","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","Rescue boat launching deck stanchions are are secured with tiger rope. KOCH SIRE inspector advised should have wire rope securing.","LSA / FFA","LSA / FFA Appliances","Inappropriate Procedure",5.1100000000000003,"Low","Not Applicable","Not Applicable"," will be done at convient.","2019-12-31",null,"Completed","2019-12-13","No",null,null,"External"]
[null,null,null,null,null,"83_15/12/2019 8:45:31 PM","2019-12-15","Other","Ship Staff","Ship Staff Insp.","About 75% of the mooring winchs \"Distance nut\" got larger value. (As the brakes are fully open, the bottom part of the brake band should rest/touch the distance nut, which is not happending due to incorrect setting).","Deck - Mooring Machinery","Mooring","Industry Issue",9.14,"Medium","Not Applicable","Not Applicable","Distance nut to be adjusted, so that it just touch when brake is fully open.","2020-01-14",null,"Completed","2020-01-15","No",null,null,"Internal"]
[null,null,null,null,null,"83_16/10/2019 6:26:56 PM","2019-04-02","Defect","Ship Staff","Ship Staff Insp.","Main engine servo leak drive rail unit alarm sensor to replace (Infront of ECR).\t\t\t","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Spare received.same renewed. working satisfactory.","2019-09-30",null,"Completed","2020-01-16","No",null,null,"Internal"]
[null,null,null,null,null,"83_17/10/2019 6:24:33 PM","2019-08-31","Defect","Ship Staff","Ship Staff Insp.","Main Engine auto back wash filter casing change over mechanism not working (both auto and manual side fuel pressure remains at any chosen change over leaver position) making filter cleaning impossible. Need to stop fuel system on main engine to clean filter.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","C/O mechanism opened up, alignment done & a locking plate arrangement made at the bottom of the C/O shaft to restrict its downward movement which was the cause of the rigid shaft.","2019-11-30"," ","Completed","2020-01-06","No",null,null,"Internal"]
[null,null,null,null,null,"83_17/1/2020 4:55:47 PM","2019-12-05","Defect","Ship Staff","Ship Staff Insp.","ME servo oil pupmp compensator solenoid valve faulty","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Spare received, same renewed. working satisfactory","2020-01-01","Requisition raised ATHE195147","Completed","2019-12-14","No",null,null,"Internal"]
[null,null,null,null,null,"83_17/10/2019 6:33:26 PM","2019-10-11","Defect","Ship Staff","Ship Staff Insp.","Air con comressor no-1 suction gas temperature sensor defective\t.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Spare received, same replaced. Working satisfactory.","2020-04-15"," Requisition ATHE190152 ","Completed","2020-01-16","No",null,null,"Internal"]
[null,null,null,null,null,"83_17/1/2020 5:05:16 PM","2019-12-13","Defect","Ship Staff","Ship Staff Insp.","# 1 ACS 2 controller, malfuntioning","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Replace the controller with a spare one, working satisfactory.","2019-12-31",null,"Completed","2019-12-14","No",null,null,"Internal"]
[null,null,null,null,null,"83_17/1/2020 5:16:59 PM","2019-11-03","Defect","Ship Staff","Ship Staff Insp.","GMDSS POWER MODULE 240 FOR inmarsat C not working","Navigation - GMDSS & Communication","Communication","Equipment Related",4.24,"High","Not Applicable","Not Applicable","Spare received, same renewed. Working satisfactory.","2019-12-31","Requisition raised ATHE195147","Completed","2019-12-23","No",null,null,"Internal"]
[null,null,null,null,null,"83_17/1/2020 5:22:42 PM","2020-01-01","Defect","Ship Staff","Ship Staff Insp.","PORT bridge wing rudder angle indicator found not working","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Broken cables renewed","2020-01-31",null,"Completed","2020-01-02","No",null,null,"Internal"]
[null,null,null,null,null,"83_21/1/2020 8:27:39 PM","2019-09-16","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Pump room start switch in CCR became faulty. Same to order and renew.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related",11.1,"Medium","Not Applicable","Not Applicable","renewed ","2019-10-15",null,"Completed","2019-10-14","No",null,null,"Internal"]
[null,null,null,null,null,"83_21/1/2020 8:30:13 PM","2019-09-16","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Soft patch on pipe catering overboard line just before overboard valve.  Pipe to remove and renew at earliest in ballast passage.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related",10.31,"Very High","Not Applicable","Not Applicable","Pipe repaired","2019-09-30",null,"Completed","2019-09-28","No",null,null,"Internal"]
[null,null,null,null,null,"83_21/1/2020 8:32:44 PM","2019-09-16","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Stern thruster electric cables to disconnect and remove.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related",10.37,"Medium","Not Applicable","Not Applicable","Done","2019-10-15",null,"Completed","2019-10-10","No",null,null,"Internal"]
[null,null,null,null,null,"83_21/1/2020 10:02:08 PM","2019-09-16","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Fuel pump LO return line / drain line to check as per RT circular 180 and report in PAL.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related",null,null,"Not Applicable","Not Applicable","Done","2019-10-15",null,"Completed","2019-12-12","No",null,null,"Internal"]
[null,null,null,null,null,"83_21/1/2020 10:06:18 PM","2019-09-08","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Fuel pumps High pressure pipes (from fuel pump till common rail) to tighten at various supports. They have tendency to crack in vibration","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related",null,null,"Not Applicable","Not Applicable","Done","2019-09-22",null,"Completed","2019-09-15","No",null,null,"Internal"]
[null,null,null,null,null,"83_21/1/2020 10:09:32 PM","2019-09-16","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Fuel pump area to clean and paint and rectify minor lo leak","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related",10.29,"Medium","Not Applicable","Not Applicable","Done","2019-09-30",null,"Completed","2019-09-25","No",null,null,"Internal"]
[null,null,null,null,null,"83_21/1/2020 10:12:23 PM","2019-09-16","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ME foundation bolt tightness to check by hyd jacks","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related",null,null,"Not Applicable","Not Applicable","Done","2019-09-30",null,"Completed","2020-01-09","No",null,null,"Internal"]
[null,null,null,null,null,"83_21/1/2020 10:15:44 PM","2019-09-16","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Steam valve for COPT governor to open and inspect for freeness. Sister vsl had trouble as valve got seized.","Cargo Mach.","Eng. / Strg. Comp.","Equipment Related",8.15,"High","Not Applicable","Not Applicable","Done","2019-09-30",null,"Completed","2019-12-03","No",null,null,"Internal"]
[null,null,null,null,null,"83_21/1/2020 10:18:34 PM","2019-09-16","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Sewage treatment plant maintenance, testing, sampling log to maintain near plant.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related",null,null,"Not Applicable","Not Applicable","Done","2019-09-23",null,"Completed","2019-09-25","No",null,null,"Internal"]
[null,null,null,null,null,"83_21/1/2020 10:24:16 PM","2019-09-16","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Terminal box for both Water ballast pp to check for tightness.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related",10.37,"Medium","Not Applicable","Not Applicable","Done","2019-09-23",null,"Completed","2019-09-30","No",null,null,"Internal"]
[null,null,null,null,null,"83_21/1/2020 10:30:49 PM","2019-09-16","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Starting air valve solenoid to blow through at regular interval (3 months) as per RT circular","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related",null,null,"Not Applicable","Not Applicable","Done","2019-10-15",null,"Completed","2019-12-21","No",null,null,"Internal"]
[null,null,null,null,null,"83_21/1/2020 10:33:41 PM","2019-09-08","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","All pipe supports for HP pipe for Exhaust valve to tighten. Unit 2 found loose.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related",null,null,"Not Applicable","Not Applicable","Done","2019-09-23",null,"Completed","2019-09-15","No",null,null,"Internal"]
[null,null,null,null,null,"83_21/1/2020 10:36:59 PM","2019-09-16","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Hyd drums in steering gear room in direct metal contact with floor. To place wood or packing.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related",10.29,"Medium","Not Applicable","Not Applicable","Done","2019-09-30",null,"Completed","2019-11-04","No",null,null,"Internal"]
[null,null,null,null,null,"83_21/1/2020 10:40:16 PM","2019-09-16","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Boiler emergency firing procedure to make and all engineers to train / familiarize.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related",null,null,"Not Applicable","Not Applicable","Done","2019-09-23",null,"Completed","2019-09-23","No",null,null,"Internal"]
[null,null,null,null,null,"83_21/1/2020 10:46:23 PM","2019-09-16","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","2 HFO bunker tanks (No 1 Stbd and No 2 Port ) to clean in upcoming voyage as per SIP . ","Hull & Tanks","Eng. / Strg. Comp.","Equipment Related",null,null,"Not Applicable","Not Applicable","Done","2019-10-15",null,"Completed","2019-10-11","No",null,null,"Internal"]
[null,null,null,null,null,"83_21/1/2020 10:48:48 PM","2019-09-16","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","To take inventory of all manuals and highlight if any missing. ","Miscellaneous","Eng. / Strg. Comp.","Equipment Related",null,null,"Not Applicable","Not Applicable","Done","2019-09-30",null,"Completed","2019-12-15","No",null,null,"Internal"]
[null,null,null,null,null,"83_21/1/2020 10:51:59 PM","2019-09-16","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Boiler pilot burner spares to order as frequently failing due to poor insulation condition.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Spares received & renewed, now pilot burner is working in good order","2019-09-30",null,"Completed","2020-01-08","No",null,null,"Internal"]
[null,null,null,null,null,"83_21/1/2020 10:56:15 PM","2019-09-16","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","COP no 3 Lub oil low pressure alarm activated at 600 rpm at 0.8 bar. The pressure switch setting to be corrected to 0.6 bar.","Cargo Mach.","Eng. / Strg. Comp.","Equipment Related",8.15,"High","Not Applicable","Not Applicable","Done","2019-09-30",null,"Completed","2019-09-19","No",null,null,"Internal"]
[null,null,null,null,null,"83_21/1/2020 10:59:26 PM","2019-09-16","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Many drain scuppers in engine room are choke. To clear them, if require cut and put flanges","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related",null,null,"Not Applicable","Not Applicable","Done","2019-12-15",null,"Completed","2019-12-20","No",null,null,"Internal"]
[null,null,null,null,null,"83_21/1/2020 11:02:28 PM","2019-09-16","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Spare HFO purifier frame to secure well on foundation in Engine room","E/R - Purifier","Eng. / Strg. Comp.","Equipment Related",null,null,"Not Applicable","Not Applicable","Purifier secured in E/R 2nd deck","2019-10-15",null,"Completed","2019-09-30","No",null,null,"Internal"]
[null,null,null,null,null,"83_21/1/2020 11:06:47 PM","2018-09-16","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","All overboard valves in Engine room to be operated manually and hydraulic pump where fitted.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related",10.31,"Very High","Not Applicable","Not Applicable","Done","2019-09-30",null,"Completed","2019-09-20","No",null,null,"Internal"]
[null,null,null,null,null,"83_21/1/2020 11:11:15 PM","2019-09-16","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Bilge pump valve seats are repaired by devcon and performance is poor. Spares on order and need urgently","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related",null,null,"Not Applicable","Not Applicable","Done","2019-10-15",null,"Completed","2019-11-01","No",null,null,"Internal"]
[null,null,null,null,null,"83_21/1/2020 11:14:10 PM","2019-09-16","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Singapore bunkering procedure guideline not onboard. To supply","Miscellaneous","Eng. / Strg. Comp.","Equipment Related",null,null,"Not Applicable","Not Applicable","Done","2019-11-15",null,"Completed","2019-12-08","No",null,null,"Internal"]
[null,null,null,null,null,"83_21/1/2020 11:17:35 PM","2019-09-16","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","PMS to incorporate spare parts from office side by Valad","Documentation","Eng. / Strg. Comp.","Equipment Related",10.119999999999999,"Very High","Not Applicable","Not Applicable","Done","2019-11-15",null,"Completed","2019-12-05","No",null,null,"Internal"]
[null,null,null,null,null,"83_21/1/2020 11:33:39 PM","2019-09-16","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","fwd & aft hyd power pack hyd hoses are leaking & requires immediate replacement.","Deck - Mooring Machinery","Mooring","Equipment Related",9.14,"Medium","Not Applicable","Not Applicable","hoses replaced with newly received hoses.","2019-09-30",null,"Completed","2019-10-04","No",null,null,"Internal"]
[null,null,null,null,null,"83_21/1/2020 11:37:01 PM","2019-09-16","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","windlass gear teeth were found dry. same to be greased.","Critical Equip.","Structural Condn. / WT integrity ","Equipment Related",9.1999999999999993,"Medium","Not Applicable","Not Applicable","windlass gear teeth greased.","2019-10-03",null,"Completed","2019-10-03","No",null,null,"Internal"]
[null,null,null,null,null,"83_21/1/2020 11:41:32 PM","2019-09-16","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","the stbd crane hydraulic hoses end connectors getting rusty. same to be brushed & apply denso tape.","Deck - Machinery","Structural Condn. / WT integrity ","Equipment Related",8.5,"Medium","Not Applicable","Not Applicable","denso tape applied at the connectors.","2019-09-18",null,"Completed","2019-09-18","No",null,null,"Internal"]
[null,null,null,null,null,"83_21/1/2020 11:45:31 PM","2019-09-16","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","stay wires to be greased & apply with denso tape.","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","Equipment Related",11.5,"Medium","Not Applicable","Not Applicable","greased & denso tape applied.","2019-09-17",null,"Completed","2019-09-17","No",null,null,"Internal"]
[null,null,null,null,null,"83_21/1/2020 11:49:24 PM","2019-09-16","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","mast riser vent valve reported leak. same to be repaired or supply new at next port.","Inert Gas","Cargo / Ballast Systems","Equipment Related",8.25,"Very High","Not Applicable","Not Applicable","defective valve replaced.","2019-09-30",null,"Completed","2019-10-01","No",null,null,"Internal"]
[null,null,null,null,null,"83_21/1/2020 11:53:23 PM","2019-09-16","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","the electric conduct line pipes are pending to be painted red brown. to complete same after surafce preparation. to supply spray painter for good quality.","Deck - Pipe / Fittings","General Appearance","Equipment Related",11.5,"Medium","Not Applicable","Not Applicable","conduvt line painting complted.","2019-12-15",null,"Completed","2019-11-09","No",null,null,"Internal"]
[null,null,null,null,null,"83_21/1/2020 11:57:03 PM","2019-09-16","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","educators to try out for various void spaces.","Deck - Machinery","Cargo / Ballast Systems","Equipment Related",8.8000000000000007,null,"Not Applicable","Not Applicable","void spaces educator tried out.","2019-10-01",null,"Completed","2019-11-01","No",null,null,"Internal"]
[null,null,null,null,null,"83_22/1/2020 12:00:31 AM","2019-09-16","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","rust spots / stains on both manifold area & its pipes to be attended.","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","Equipment Related",11.4,"Very High","Not Applicable","Not Applicable","derusting & painting of manifold area pipes carried out.","2019-10-15",null,"Completed","2019-10-16","No",null,null,"Internal"]
[null,null,null,null,null,"83_22/1/2020 12:03:18 AM","2019-09-16","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","few mooring wires found lacking grease.","Deck - Mooring Machinery","Mooring","Equipment Related",9.17,"High","Not Applicable","Not Applicable","mooring wires greased.","2019-10-15",null,"Completed","2019-10-09","No",null,null,"Internal"]
[null,null,null,null,null,"83_22/1/2020 12:06:57 AM","2019-09-16","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","life boat davit RAM pin grease points dry, same to grease.","LSA / FFA","Emgcy. Systems","Equipment Related",5.29,"High","Not Applicable","Not Applicable","greasing carried out.","2019-09-30",null,"Completed","2019-10-19","No",null,null,"Internal"]
[null,null,null,null,null,"83_22/1/2020 12:11:06 AM","2019-09-16","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","the rope retaining the life boat grab wires should be secured properly so that it can be released quickly after launching.","LSA / FFA","Emgcy. Systems","Equipment Related",5.29,"High","Not Applicable","Not Applicable","job completed.","2019-09-30",null,"Completed","2019-10-18","No",null,null,"Internal"]
[null,null,null,null,null,"83_22/1/2020 12:18:45 AM","2019-09-16","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","gangway air lubricator for stbd side to renew with onboard spare.","Deck - Machinery","Structural Condn. / WT integrity ","Equipment Related",5.47,"Medium","Not Applicable","Not Applicable","air lubricator renewed.","2019-09-30",null,"Completed","2019-10-03","No",null,null,"Internal"]
[null,null,null,null,null,"83_22/1/2020 12:21:32 AM","2019-09-16","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp."," M4 winch control block is cut & repaired. same to order & replace.M","Deck - Mooring Machinery","Mooring","Equipment Related",9.17,"High","Not Applicable","Not Applicable","control block replaced.","2019-12-15",null,"Completed","2019-12-10","No",null,null,"Internal"]
[null,null,null,null,null,"83_22/1/2020 12:27:37 AM","2019-09-16","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Crew requested entertainment items, same to be supplied at convient port.","Miscellaneous","Crew Management","Behaviour Based",11.8,"Low","Not Applicable","Not Applicable","supplied.","2019-09-30",null,"Completed","2019-09-24","No",null,null,"Internal"]
[null,null,null,null,null,"83_22/1/2020 12:30:58 AM","2019-09-16","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ventilator fan to derust & paint.","Deck - Machinery","Structural Condn. / WT integrity ","Equipment Related",11.7,"High","Not Applicable","Not Applicable","derusted & painted.","2019-09-30",null,"Completed","2019-10-14","No",null,null,"Internal"]
[null,null,null,null,null,"83_22/1/2020 12:36:06 AM","2019-09-16","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","life raft embarkation ladder canvas cover is torn & performance is poor.","LSA / FFA","LSA / FFA Appliances","Inappropriate Procedure",5.14,"Very High","Not Applicable","Not Applicable","completd","2019-09-30",null,"Completed","2019-10-02","No",null,null,"Internal"]

{"sheet":"Calc","index":2,"n_rows":28,"n_cols":12,"rows_kept":28,"cut":false,"hidden":true,"merged":[]}
["Def_type","Def_cause","Equipments","VIQrefno","Observer_code"]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,"Dim itemSele As Long"]
[null,null,null,null,null,null,null,null,null,null,null,"   dim startRow as integer"]
[null,null,null,null,null,null,null,null,null,null,null,"   startRow=1"]
[null,null,null,null,null,null,null,null,null,null,null,"        For itemSele = 0 To ListBox1.ListCount - 1"]
[null,null,null,null,null,null,null,null,null,null,null,"        If ListBox1.Selected(itemSele) = True Then"]
[null,null,null,null,null,null,null,null,null,null,null,"        Worksheets(\"WorksheetName\").Range(\"A\" & startRow).Value = ListBox1.List(itemSele)"]
[null,null,null,null,null,null,null,null,null,null,null,"        startRow = startRow + 1"]
[null,null,null,null,null,null,null,null,null,null,null,"        End If"]
[null,null,null,null,null,null,null,null,null,null,null,"        Next"]
[null,null,null,null,null,null,null,null,null,null,null,"Dim LastRowA As String"]
[null,null,null,null,null,null,null,null,null,null,null,"        Dim itemSele As Long"]
[null,null,null,null,null,null,null,null,null,null,null,"       Dim startRow as integer"]
[null,null,null,null,null,null,null,null,null,null,null,"        LastRowA = ActiveSheet.Cells(Rows.count, \"A\").End(xlUp).row"]
[null,null,null,null,null,null,null,null,null,null,null,"        startQue = 0"]
[null,null,null,null,null,null,null,null,null,null,null,"        For itemSele = 0 To ListBox1.ListCount - 1"]
[null,null,null,null,null,null,null,null,null,null,null,"        For startRow = 1 To LastRowA"]
[null,null,null,null,null,null,null,null,null,null,null,"        If Worksheets(\"WorksheetName\").Range(\"A\" & startRow).Value = ListBox1.List(itemSele) Then"]
[null,null,null,null,null,null,null,null,null,null,null,"        ListBox1.Selected(itemSele) = True"]
[null,null,null,null,null,null,null,null,null,null,null,"        Exit For"]
[null,null,null,null,null,null,null,null,null,null,null,"        End If"]
[null,null,null,null,null,null,null,null,null,null,null,"        Next j"]
[null,null,null,null,null,null,null,null,null,null,null,"        Next"]
[null,null,null,null,null,null,null,null,null,null,null,"        End If"]

{"sheet":"Areaofobs","index":3,"n_rows":17,"n_cols":2,"rows_kept":17,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Cargo / Ballast Systems",11]
["Cert. & Docu.",2]
["Communication",6]
["Crew Management",3]
["Emgcy. Systems",13]
["Eng. / Strg. Comp.",14]
["General Appearance",15]
["Ice Opns.",17]
["ISM Related",7]
["ISPS Related",10]
["LSA / FFA Appliances",8]
["MARPOL Related",9]
["MLC Related",4]
["Mooring",12]
["Navigation",5]
["Structural Condn. / WT integrity ",16]

{"sheet":"Vessel_type","index":4,"n_rows":1,"n_cols":2,"rows_kept":1,"cut":false,"hidden":true,"merged":[]}
["Vessel_type","ID"]

{"sheet":"Deficiency_type","index":5,"n_rows":8,"n_cols":3,"rows_kept":8,"cut":false,"hidden":true,"merged":[]}
["TITLE","Type of deficiency_description","ID"]
["Breakdown",null,6]
["Critical Equipment",null,4]
["Defect",null,1]
["Guarantee Claim",null,8]
["Non Conformity",null,2]
["Observation",null,3]
["Other",null,7]

{"sheet":"VIQrefno","index":6,"n_rows":427,"n_cols":3,"rows_kept":427,"cut":false,"hidden":true,"merged":[]}
["VIQ_ref_no","Risk Value of observation","ID"]
["1.1","Low",8243]
["1.10","Low",8252]
["1.11","Low",8253]
["1.12","Low",8254]
["1.13","Low",8255]
["1.14","Low",8256]
["1.15","Low",8257]
["1.16","Low",8259]
["1.17","Low",8260]
["1.18","Low",8261]
["1.19","Low",8262]
["1.2","Low",8244]
["1.20","Low",8263]
["1.21","Low",8265]
["1.22","Low",8266]
["1.23","Low",8267]
["1.24","Low",8268]
["1.25","Low",8269]
["1.26","Low",8270]
["1.3","Low",8245]
["1.4","Low",8246]
["1.5","Low",8247]
["1.6","Low",8248]
["1.7","Low",8249]
["1.8","Low",8250]
["1.9","Low",8251]
["1.99","High",11258]
["10.1","Medium",8461]
["10.10","High",8470]
["10.11","Medium",8471]
["10.12","Very High",8472]
["10.13","Very High",8473]
["10.14","Medium",8474]
["10.15","Low",8475]
["10.16","Very High",8476]
["10.17","Very High",8477]
["10.18","High",8478]
["10.19","Very High",8479]
["10.2","Low",8462]
["10.20","High",8480]
["10.21","Medium",8481]
["10.22","Low",8482]
["10.23","Medium",8483]
["10.24","Low",8484]
["10.25","Very High",8485]
["10.26","High",8486]
["10.27","Medium",8487]
["10.28","Low",8488]
["10.29","Medium",8489]
["10.3","Medium",8463]
["10.30","High",8490]
["10.31","Very High",8491]
["10.32","Very High",8492]
["10.33","High",8493]
["10.34","High",8494]
["10.35","Very High",8495]
["10.36","Very High",8496]
["10.37","Medium",8497]
["10.38","Medium",8498]
["10.39","High",8499]
["10.4","High",8464]
["10.40","Medium",8500]
["10.41","Medium",8501]
["10.42","Medium",8502]
["10.43","Medium",8503]
["10.44","Medium",8504]
["10.45","Very High",8505]
["10.46","High",8506]
["10.47","Medium",8507]
["10.48","High",8508]
["10.49","Medium",8509]
["10.5","Low",8465]
["10.50","High",8510]
["10.51","Low",8511]
["10.52","Medium",8512]
["10.53","Medium",8513]
["10.54","High",8514]
["10.55","Low",8515]
["10.6","Very High",8466]
["10.7","Medium",8467]
["10.8","Medium",8468]
["10.9","Medium",8469]
["10.99","High",8516]
["11.1","High",8420]
["11.10","Medium",8429]
["11.11","Very High",8430]
["11.12","Low",8431]
["11.13","Low",8432]
["11.14","Medium",8433]
["11.15","Low",8434]
["11.16","Low",8435]
["11.17","Low",8436]
["11.2","Medium",8421]
["11.3","Medium",8422]
["11.4","Very High",8423]
["11.5","Medium",8424]
["11.6","Medium",8425]
["11.7","High",8426]
["11.8","Low",8427]
["11.9","Low",8428]
["11.99","High",8437]
["12.1","High",8438]
["12.10","High",8448]
["12.11","High",8449]
["12.12","High",8450]
["12.13","High",8451]
["12.14","High",8452]
["12.15","High",8453]
["12.16","High",8454]
["12.17","High",8455]
["12.18","High",8456]
["12.19","High",8457]
["12.2","High",8439]
["12.20","High",8458]
["12.21","High",8459]
["12.3","High",8441]
["12.4","High",8442]
["12.5","High",8443]
["12.6","High",8444]
["12.7","High",8445]
["12.8","High",8446]
["12.9","High",8447]
["12.99","High",8460]
["2.1","Very High",8296]
["2.1.9","Very High",11259]
["2.10","Medium",8304]
["2.11","Medium",8305]
["2.12","Low",8306]
["2.13","Low",8307]
["2.14","Low",8308]
["2.15","Low",8309]
["2.16","Medium",8310]
["2.2","Medium",8297]
["2.3","High",8295]
["2.4","Medium",8298]
["2.5","Medium",8299]
["2.6","Low",8300]
["2.7","High",8301]
["2.8","High",8302]
["2.9","Medium",8303]
["2.99","High",8311]
["3.1","High",8312]
["3.2","Very High",8313]
["3.3","High",8314]
["3.4","Low",8294]
["3.5","Medium",8315]
["3.6","High",8316]
["3.7","Very High",8317]
["3.8","Very High",8318]
["3.99","High",8319]
["4.1","High",8320]
["4.10","High",8329]
["4.11","Medium",8330]
["4.12","Very High",8331]
["4.13","Very High",8332]
["4.14","Very High",8333]
["4.15","Very High",8334]
["4.16","Very High",8335]
["4.17","Very High",8336]
["4.18","Very High",8337]
["4.19","Low",8338]
["4.2","Medium",8321]
["4.20","Very High",8339]
["4.21","High",8340]
["4.22","Low",8341]
["4.23","High",8342]
["4.24","High",8343]
["4.25","Low",8344]
["4.26","Low",8345]
["4.27","High",8346]
["4.3","Medium",8322]
["4.4","High",8323]
["4.5","Very High",8324]
["4.6","Medium",8325]
["4.7","High",8326]
["4.8","Medium",8327]
["4.9","Medium",8328]
["4.99","High",8347]
["5.1","Very High",8517]
["5.10","High",8526]
["5.11","Low",8527]
["5.12","Medium",8528]
["5.13","High",8529]
["5.14","Very High",8530]
["5.15","Medium",8531]
["5.16","Very High",8532]
["5.17","Very High",8533]
["5.18","High",8534]
["5.19","Medium",8535]
["5.2","Very High",8518]
["5.20","Medium",8536]
["5.21","Medium",8537]
["5.22","High",8539]
["5.23","Very High",8540]
["5.24","Very High",8541]
["5.25","Medium",8542]
["5.26","Medium",8543]
["5.27","Medium",8544]
["5.28","Very High",8545]
["5.29","High",8546]
["5.3","Low",8519]
["5.30","High",8547]
["5.31","High",8548]
["5.32","High",8549]
["5.33","High",8550]
["5.34","Low",8551]
["5.35","Medium",8552]
["5.36","Low",8553]
["5.37","Low",8554]
["5.38","High",8555]
["5.39","Very High",8556]
["5.4","High",8520]
["5.40","Very High",8557]
["5.41","Very High",8558]
["5.42","Medium",8559]
["5.43","High",8560]
["5.44","High",8561]
["5.45","Medium",8564]
["5.46","Medium",8565]
["5.47","Medium",8566]
["5.48","Medium",8567]
["5.5","Low",8521]
["5.6","Low",8522]
["5.7","Medium",8523]
["5.8","Medium",8524]
["5.9","Very High",8525]
["5.99","High",8568]
["6.1","Medium",8348]
["6.10","Low",8357]
["6.11","High",8358]
["6.12","Medium",8359]
["6.13","Low",8360]
["6.14","High",8361]
["6.15","High",8362]
["6.16","Very High",8363]
["6.17","Very High",8364]
["6.18","Medium",8365]
["6.19","Low",8366]
["6.2","High",8349]
["6.20","Medium",8367]
["6.21","High",8368]
["6.22","Medium",8369]
["6.3","Low",8350]
["6.4","High",8351]
["6.5","Medium",8352]
["6.6","Medium",8353]
["6.7","High",8354]
["6.8","High",8355]
["6.9","Low",8356]
["6.99","High",8370]
["7.1","High",8371]
["7.10","High",8380]
["7.11","High",8381]
["7.12","High",8382]
["7.13","Medium",8383]
["7.14","Medium",8384]
["7.15","High",8385]
["7.16","High",8386]
["7.17","High",8387]
["7.2","High",8372]
["7.3","Low",8373]
["7.4","Low",8374]
["7.5","Low",8375]
["7.6","Medium",8376]
["7.7","Low",8377]
["7.8","High",8378]
["7.9","High",8379]
["7.99","High",8388]
["8.1","Very High",8569]
["8.10","Very High",8578]
["8.100","Low",11227]
["8.101","Medium",11228]
["8.102","Low",11229]
["8.103","Low",11230]
["8.104","Low",11231]
["8.105","Medium",11232]
["8.106","Medium",11233]
["8.107","Low",11234]
["8.108","High",11235]
["8.109","Very High",11236]
["8.11","Medium",8579]
["8.110","High",11237]
["8.111","Medium",11238]
["8.112","High",11239]
["8.113","Medium",11240]
["8.114","Low",11241]
["8.115","High",11242]
["8.116","Medium",11243]
["8.117","Medium",11244]
["8.118","Medium",11245]
["8.119","High",11246]
["8.12","Medium",8580]
["8.120","High",11247]
["8.121","Medium",11248]
["8.122","High",11249]
["8.123","High",11250]
["8.124","Low",11251]
["8.125","High",11252]
["8.126","Medium",11253]
["8.127","Medium",11254]
["8.13","Medium",8581]
["8.14","Very High",8582]
["8.15","High",8583]
["8.16","Very High",8584]
["8.17","Low",8585]
["8.18","High",8586]
["8.19","High",8587]
["8.199","High",11255]
["8.2","Medium",8570]
["8.20","Medium",8588]
["8.21","High",8589]
["8.22","Very High",8590]
["8.23","Medium",8591]
["8.24","Medium",8592]
["8.25","Very High",8593]
["8.26","High",8594]
["8.27","Medium",8595]
["8.28","Medium",8596]
["8.29","High",8598]
["8.3","Very High",8571]
["8.30","High",8599]
["8.31","High",8600]
["8.32","Low",8601]
["8.33","Medium",8602]
["8.34","High",8603]
["8.35","Medium",8604]
["8.36","Medium",8605]
["8.37","High",8607]
["8.38","Medium",8608]
["8.39","Medium",8609]
["8.4","Medium",8572]
["8.40","High",8610]
["8.41","Medium",8611]
["8.42","Medium",8612]
["8.43","Very High",8613]
["8.44","High",8615]
["8.45","High",8616]
["8.46","Very High",8617]
["8.47","Very High",8618]
["8.48","Medium",8619]
["8.49","High",8620]
["8.5","Very High",8573]
["8.50","Medium",8621]
["8.51","Low",8622]
["8.52","Low",8623]
["8.53","Low",8624]
["8.54","High",8625]
["8.55","Low",11182]
["8.56","Medium",11183]
["8.57","Medium",11184]
["8.58","High",11185]
["8.59","High",11186]
["8.6","Medium",8574]
["8.60","High",11187]
["8.61","Medium",11188]
["8.62","Very High",11189]
["8.63","High",11190]
["8.64","Medium",11191]
["8.65","Low",11192]
["8.66","High",11193]
["8.67","High",11194]
["8.68","High",11195]
["8.69","Medium",11196]
["8.7","High",8575]
["8.70","Medium",11197]
["8.71","Very High",11198]
["8.72","Medium",11199]
["8.73","Medium",11200]
["8.74","High",11201]
["8.75","Medium",11202]
["8.76","Medium",11203]
["8.77","Medium",11204]
["8.78","Medium",11205]
["8.79","Medium",11206]
["8.8","Medium",8576]
["8.80","Medium",11207]
["8.81","Low",11208]
["8.82","Medium",11209]
["8.83","Low",11210]
["8.84","Low",11211]
["8.85","Medium",11212]
["8.86","Medium",11213]
["8.87","Medium",11214]
["8.88","Low",11215]
["8.89","High",11216]
["8.9","High",8577]
["8.90","High",11217]
["8.91","High",11218]
["8.92","Medium",11219]
["8.93","Low",11220]
["8.94","Low",11221]
["8.95","Medium",11222]
["8.96","Medium",11223]
["8.97","Low",11224]
["8.98","High",11225]
["8.99","Medium",11226]
["9.1","Low",8390]
["9.10","Medium",8399]
["9.11","Medium",8400]
["9.12","Medium",8401]
["9.13","Low",8402]
["9.14","Medium",8403]
["9.15","Medium",8404]
["9.16","High",8405]
["9.17","High",8406]
["9.18","Low",8407]
["9.19","Low",8408]
["9.2","Very High",8391]
["9.20","Medium",8409]
["9.21","Medium",8410]
["9.22","Low",8411]
["9.23","Low",8412]
["9.24","Medium",8413]
["9.25","Low",8414]
["9.26","Low",8415]
["9.27","Low",8416]
["9.28","Medium",8417]
["9.29","Low",8418]
["9.3","Very High",8392]
["9.4","High",8393]
["9.5","High",8394]
["9.6","Low",8395]
["9.7","Medium",8396]
["9.8","Medium",8397]
["9.9","Medium",8398]
["9.99","High",8419]

{"sheet":"Equipment_list","index":7,"n_rows":27,"n_cols":3,"rows_kept":27,"cut":false,"hidden":true,"merged":[]}
["TITLE","Equipment_list_description","ID"]
["Accommodation ",null,12]
["Cargo Mach.",null,13]
["Critical Equip.",null,16]
["Deck - Machinery",null,18]
["Deck - Mooring Machinery",null,15]
["Deck - Pipe / Fittings",null,20]
["Documentation",null,21]
["E/R - Air Comp.",null,8]
["E/R - Aux. Engine",null,4]
["E/R - Aux. Mach.",null,7]
["E/R - Boiler",null,5]
["E/R - Main Engine",null,3]
["E/R - Pipes/ valves & fittings",null,9]
["E/R - Purifier",null,6]
["Elect. Mach. & Equip.",null,10]
["Hull & Tanks",null,19]
["Inert Gas",null,14]
["LSA / FFA",null,17]
["Miscellaneous",null,22]
["Navigation - DGPS / EPFS / AIS",null,28]
["Navigation - ECDIS",null,25]
["Navigation - Echo Sounder / Speed Log",null,26]
["Navigation - GMDSS & Communication",null,23]
["Navigation - Others",null,11]
["Navigation - RADAR",null,24]
["Navigation - VDR / BNWAS",null,30]

{"sheet":"PSC_MOU","index":8,"n_rows":11,"n_cols":3,"rows_kept":11,"cut":false,"hidden":true,"merged":[]}
["TITLE","PSC_MOU_description","ID"]
["Asia and the Pacific",null,2]
["Caribbean",null,4]
["Europe and the North Atlantic",null,1]
["Latin America",null,3]
["The Black Sea region",null,6]
["The Indian Ocean",null,8]
["The Mediterranean",null,7]
["The Riyadh MoU",null,9]
["USCG",null,10]
["West and Central Africa",null,5]

{"sheet":"Inspection_type","index":9,"n_rows":11,"n_cols":2,"rows_kept":11,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Bunkering Audit",14]
["Engineering Audit",16]
["ISM Audit",2]
["ISPS Audit",3]
["IT Audit",10]
["MLC Audit",1]
["Mooring Audit",9]
["Nav Audit / Verification",8]
["Ship Staff Insp.",15]
["Suptd. Insp.",13]

{"sheet":"Deficiency_Cause","index":10,"n_rows":8,"n_cols":3,"rows_kept":8,"cut":false,"hidden":true,"merged":[]}
["TITLE","Deficiency_Cause_description","ID"]
["Behaviour Based",null,1]
["Equipment Related",null,4]
["External Factors",null,5]
["Human Error",null,7]
["Inappropriate Procedure",null,8]
["Industry Issue",null,6]
["Knowledge Based",null,3]

{"sheet":"Observer_code","index":11,"n_rows":3,"n_cols":3,"rows_kept":3,"cut":false,"hidden":true,"merged":[]}
["TITLE","Observer_code_description","ID"]
["Owner / Marine / Tech. Suptd.",null,3]
["Ship Staff",null,2]

{"sheet":"Status_code","index":12,"n_rows":6,"n_cols":3,"rows_kept":6,"cut":false,"hidden":true,"merged":[]}
["TITLE","Status_code_description","ID"]
["Completed",null,6]
["Deferred to D D",null,5]
["In progress",null,3]
["Not Started",null,2]
["Waiting spare",null,4]

{"sheet":"PSC_ref_no","index":13,"n_rows":19,"n_cols":2,"rows_kept":19,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Alarms",9]
["Cargo operations including equipment",7]
["Certificates & Documentation",2]
["Dangerous Goods",13]
["Emergency Systems",5]
["Fire safety",8]
["ISM",16]
["ISPS",17]
["Life saving appliances",12]
["MLC, 2006",18]
["Other",19]
["Pollution Prevention",15]
["Propulsion and auxiliary machinery",14]
["Radio communication",6]
["Safety of Navigation",11]
["Structural condition",3]
["Water/Weathertight condition",4]
["Working and Living Conditions",10]

{"sheet":"Risk_value_of_obs","index":14,"n_rows":1,"n_cols":2,"rows_kept":1,"cut":false,"hidden":true,"merged":[]}
["Risk Value of observation","ID"]

{"sheet":"Year","index":15,"n_rows":18,"n_cols":1,"rows_kept":18,"cut":false,"hidden":true,"merged":[]}
["Year"]
[2014]
[2015]
[2016]
[2017]
[2018]
[2019]
[2020]
[2021]
[2022]
[2023]
[2024]
[2025]
[2026]
[2027]
[2028]
[2029]
[2030]

{"sheet":"Month","index":16,"n_rows":13,"n_cols":1,"rows_kept":13,"cut":false,"hidden":true,"merged":[]}
["Month"]
["Jan"]
["Feb"]
["Mar"]
["Apr"]
["May"]
["Jun"]
["Jul"]
["Aug"]
["Sep"]
["Oct"]
["Nov"]
["Dec"]

{"sheet":"Date_","index":17,"n_rows":32,"n_cols":1,"rows_kept":32,"cut":false,"hidden":true,"merged":[]}
["Date"]
["01"]
["02"]
["03"]
["04"]
["05"]
["06"]
["07"]
["08"]
["09"]
[10]
[11]
[12]
[13]
[14]
[15]
[16]
[17]
[18]
[19]
[20]
[21]
[22]
[23]
[24]
[25]
[26]
[27]
[28]
[29]
[30]
[31]

{"sheet":"Sheet1","index":18,"n_rows":24,"n_cols":6,"rows_kept":24,"cut":false,"hidden":true,"merged":[]}
[]
[null,"ID","E",null,"Date Recorded",1]
[null,"UNIQUE ID","F",null,"Type of Deficiency",2]
[1,"Date Recorded","G",null,"Observer code",3]
["ignore","Vessel Type","H",null,"Type of Inspection",4]
[null,"Internal / External","I",null,"Description of Deficiency",5]
[null,"Drydock","J",null,"Equipment Categories",6]
[null,"Information Sharing","K",null,"Area of Observation",7]
[null,"Critical_item","L",null,"Deficiency Cause",8]
[null,"Deficiency Type","M",null,"VIQ Ref Number",9]
[null,"Deficiency Cause","N",null,"Risk Value of Obs",10]
[null,"Inspection Type","O",null,"PSC Ref Number",11]
[null,"Equipments","P",null,"PSC MOU ID",12]
[null,"VIQ Reference Number","Q",null,"Action Taken or Required",13]
[null,"Risk Value of the observation","R",null,"Target Date",14]
[null,"PSC Reference Number","S",null,"PO Ref No.",15]
[null,"PSC MOU","T",null,"Status Code",16]
[null,"Observer Code","U",null,"Date Completed",17]
[null,"Target Date","V",null,"Drydock",18]
[null,"Status Code","W",null,"Info Sharing",19]
[null,"Description of Deficiency","X",null,"Critical Item Flag",20]
[null,"Action taken / required","Y",null,"Audit Type",21]
[null,"PO ref no","Z"]
[null,"Date completed","AA"]

{"sheet":"Ship_information","index":19,"n_rows":2,"n_cols":3,"rows_kept":2,"cut":false,"hidden":true,"merged":[]}
["Ship_ID","Ship_Name","FILE_NAME"]
["83","ATHERINA (26-12-2019)","83_1577775859158.xlsm"]

{"sheet":"External_Deficiency_type","index":20,"n_rows":5,"n_cols":3,"rows_kept":5,"cut":false,"hidden":true,"merged":[]}
["TITLE","Type of deficiency_description","ID"]
["Condn of Class / Memo",null,5]
["Defect",null,1]
["Non Conformity",null,2]
["Observation",null,3]

{"sheet":"External_Inspection_type","index":21,"n_rows":10,"n_cols":2,"rows_kept":10,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Flag State Insp.",5]
["ISM Audit",2]
["ISPS Audit",3]
["MLC Audit",1]
["Nav Audit / Verification",8]
["OM Insp. (Eg. SIRE / CDI etc.)",6]
["Others (Eg. Insurance etc.)",12]
["PSC Inspection",4]
["Terminal Insp.",11]

{"sheet":"External_Observer_code","index":22,"n_rows":7,"n_cols":3,"rows_kept":7,"cut":false,"hidden":true,"merged":[]}
["TITLE","Observer_code_description","ID"]
["Class Surveyor",null,4]
["FSC Inspector",null,5]
["Others (Eg. Insurance etc.)",null,9]
["PSC Insp.",null,6]
["SIRE / CDI Insp.",null,8]
["Terminal Insp.",null,7]

{"sheet":"Sheet Version","index":23,"n_rows":2,"n_cols":2,"rows_kept":2,"cut":false,"hidden":true,"merged":[]}
["Version","Title"]
["2.0","Version 2.0"]