{"text_format":"1","workbook":"xlsx","n_sheets":24,"sheets":["Mainsheet","Completed","Calc","Areaofobs","Vessel_type","Deficiency_type","VIQrefno","Equipment_list","PSC_MOU","Inspection_type","Deficiency_Cause","Observer_code","Status_code","PSC_ref_no","Risk_value_of_obs","Year","Month","Date_","Sheet1","Ship_information","External_Deficiency_type","External_Inspection_type","External_Observer_code","Sheet Version"],"not_rendered":{"charts":0,"images":5,"macros":1,"external_links":0,"defined_names":12,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Mainsheet","index":0,"n_rows":20,"n_cols":28,"rows_kept":20,"cut":false,"hidden":false,"merged":[[10,8,10,9],[10,12,10,13],[12,6,12,27],[8,6,8,27]]}
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,"Defect - Damage Monitoring Sheet"]
[]
[null,null,null,null,null,null,null,"Date of Report","19-Mar-2020",null,null,"Ship Name","VIRGO (21-01-2020)"]
[]
[null,null,null,null,null,null,"VERSION : 2.0"]
[]
[]
[]
[null,null,null,null,"ID","UNIQUE ID","Date Recorded","Type of Deficiency","Observer code","Type of Inspection","Description of Deficiency","Equipment Categories","Area of Observation","Deficiency Cause","VIQ Ref Number","Risk Value of Obs","PSC Ref Number","PSC MOU ID","Action Taken or Required","Target Date","PO Ref No.","Status Code","Date Completed","Drydock","Info Sharing","Critical Item","Audit Type","Superintendent Remarks"]
[null,null,null,null,null,"86_05-04-2020 11:26:01","2020-01-15","Defect","Ship Staff","Ship Staff Insp.","Loadicator not working in online mode","Critical Equip.","Cargo / Ballast Systems","Equipment Related",null,null,"Not Applicable","Not Applicable","Requisition for spares raised","2020-04-30",null,"In progress",null,"No",null,null,"Internal"]
[null,null,null,null,null,"86_05-04-2020 13:16:24","2020-02-08","Defect","Ship Staff","Ship Staff Insp.","baLLAST WATER SYSTEM FOR ENGINE ROOM AFT PEAK TANK BALLASTING AND DEBALLASTING FLOW CONTROL VALVE NOT OPERATING IN AUTO MADE","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related",null,null,"Not Applicable","Not Applicable","TRIED OUT AS PER INSTRUCTIONS GIVEN BY MAKER THE WORK IS STILL IN PROGRESS","2020-04-22",null,"In progress",null,"No",null,null,"Internal"]
[null,null,null,null,null,"86_05-04-2020 11:29:43","2020-04-01","Observation","Ship Staff","Ship Staff Insp.","Hose handling crane Nut Bolts, Spring Washer / Lock Washer are of MS material ","Deck - Machinery","Cargo / Ballast Systems","Equipment Related",null,null,"Not Applicable","Not Applicable","Requisition raised for SUS 316 Spring Washer / Lock Washer","2020-06-30",null,"Waiting spare",null,"No",null,null,"Internal"]

{"sheet":"Completed","index":1,"n_rows":241,"n_cols":28,"rows_kept":241,"cut":false,"hidden":false,"merged":[[10,8,10,9],[10,12,10,13],[12,6,12,27],[8,6,8,27]]}
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,"Defect - Damage Monitoring Sheet"]
[]
[null,null,null,null,null,null,null,"Date of Report","19-Mar-2020",null,null,"Ship Name","VIRGO (21-01-2020)"]
[]
[null,null,null,null,null,null,"VERSION : 2.0"]
[]
[]
[]
[null,null,null,null,"ID","UNIQUE ID","Date Recorded","Type of Deficiency","Observer code","Type of Inspection","Description of Deficiency","Equipment Categories","Area of Observation","Deficiency Cause","VIQ Ref Number","Risk Value of Obs","PSC Ref Number","PSC MOU ID","Action Taken or Required","Target Date","PO Ref No.","Status Code","Date Completed","Drydock","Info Sharing","Critical Item","Audit Type","Superintendent Remarks"]
[null,null,null,null,8519,"86_Tue Oct 08 2019 17:13:26 GMT+0000 (Coordinated Universal Time)","2019-06-14","Defect","Ship Staff","Ship Staff Insp.","Few of Bunker and Ballast tanks sounding caps was not fitting tightly","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","Equipment Related","8.38","Low","","","All Ballast and Bunker Tanks sounding caps taken our removed old greased and chipped and made fitt to the sounding pipe ","2019-07-14","NA","Completed","2019-09-14","No","No","No","Internal"]
[null,null,null,null,3057,"86_2019-10-08 17:13:26.999","2019-06-14","Defect","Ship Staff","Ship Staff Insp.","Few of Bunker and Ballast tanks sounding caps was not fitting tightly","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","Equipment Related","8.38","Low","","","All Ballast and Bunker Tanks sounding caps taken our removed old greased and chipped and made fitt to the sounding pipe ","2019-07-14","NA","Completed","2019-09-14","No","No","No","Internal"]
[null,null,null,null,3093,"86_2019-08-10 14:55:29.000","2019-06-28","Defect","Ship Staff","Ship Staff Insp.","Spot rust around Bay area, Pipe support,cable support and beneath gratings","Deck - Pipe / Fittings","General Appearance","Inappropriate Procedure","11.6","Medium","","","De-Rusting and Painting around Bay area, Pipe support,cable support and beneath gratings carried out till midship area","2019-11-30","","Completed","2020-01-15","No","No","No","Internal"]
[null,null,null,null,3094,"86_2019-09-10 09:10:52.000","2019-06-28","Defect","Ship Staff","Ship Staff Insp.","STEAM BRANCH LINE AT HEAT EXCHANGER HEAVILY CORRODED AND BROKEN","Deck - Pipe / Fittings","General Appearance","Inappropriate Procedure","11.6","Medium","","","CORRODED STEAM BRANCH LINES RENEWED IN DRYDOCK ","2019-07-28","","Completed","2020-01-10","No","No","No","Internal"]
[null,null,null,null,3095,"86_2019-09-10 09:14:11.999","2019-06-28","Defect","Ship Staff","Ship Staff Insp.","SOPT RUST ON STEAM BRANCH LINES THROUGHOUT THE SHIP","Deck - Pipe / Fittings","General Appearance","Inappropriate Procedure","11.6","Medium","","","DE-RUSTING CARRIED OUT ON CORRODED AREAS. DAMAGED PIPELINES RENEWED ","2019-07-28","","Completed","2020-01-10","No","No","No","Internal"]
[null,null,null,null,3096,"86_2019-09-10 09:42:59.000","2019-06-28","Defect","Ship Staff","Ship Staff Insp.","FOAM LINE ,FIRE LINE STEAM LINE ,IG LINE , SPOT RUST AT THE BOTTOM OF THE PIPE THROUGHOUT THE SHIPS LENGTH, INCLUDING THE BRANCH LINE CLAMPS ARE ALSO RUSTED","Deck - Pipe / Fittings","General Appearance","Inappropriate Procedure","11.6","Medium","","","SPOT DERUSTING AND PAINTING OF PIPELINES CARRIED OUT ","2019-07-28","","Completed","2019-12-05","No","No","No","Internal"]
[null,null,null,null,3097,"86_2019-09-10 09:46:29.000","2019-06-28","Defect","Ship Staff","Ship Staff Insp.","BUNKER MANIFOLD PRESENTATION FLANGE NOT IN GOOD CONDITION","Deck - Pipe / Fittings","General Appearance","Inappropriate Procedure","","","","","FLANGE FABRICATED, AND FIXED BACK","2019-07-28","","Completed","2019-08-08","No","No","No","Internal"]
[null,null,null,null,3098,"86_2019-09-10 09:51:49.000","2019-06-28","Defect","Ship Staff","Ship Staff Insp.","TRACES OF LEAKAGE FOUND AT ALL FOAM MONITOR SEAL","LSA / FFA","Safety / LSA / FFA","Inappropriate Procedure","5.35","Medium","","","OVERHAULING OF FOAM MONITORS CARRIED OUT. ","2019-07-28","","Completed","2019-12-25","No","No","No","Internal"]
[null,null,null,null,3100,"86_2019-09-10 10:24:04.000","2019-06-28","Defect,Defect","Ship Staff","Ship Staff Insp.","PORT SIDE EYE WASH DRAIN VALVE NOT HOLDING","LSA / FFA","Safety / LSA / FFA","Inappropriate Procedure","","","","","DRAIN VALVE RENEWED IN DRYDOCK ","2019-07-29","","Completed","2020-01-05","No","No","No","Internal"]
[null,null,null,null,3101,"86_2019-09-10 10:20:25.999","2019-06-28","Defect","Ship Staff","Ship Staff Insp.","BALLAST TANK LEVEL GAUGE SHOWING INCORRECT READINGS IN CCR","Cargo Mach.","Cargo / Ballast Systems","Inappropriate Procedure","8.8","Very High","","","BALLAST TANK SENSORS RENEWED IN DRYDOCK. ","2019-07-29","","Completed","2020-01-12","No","No","No","Internal"]
[null,null,null,null,8490,"86_Sat Aug 10 2019 14:55:29 GMT+0000 (Coordinated Universal Time)","2019-06-28","Defect","Ship Staff","Ship Staff Insp.","Spot rust around Bay area, Pipe support,cable support and beneath gratings","Deck - Pipe / Fittings","General Appearance","Inappropriate Procedure","11.6","Medium","","","De- Rusting and painting around Bay area, Pipe support,cable support and beneath gratings carried out till midship areas.","2019-11-30","","Completed","2019-10-14","No","No","No","Internal"]
[null,null,null,null,8491,"86_Wed Oct 09 2019 09:10:52 GMT+0000 (Coordinated Universal Time)","2019-06-28","Defect","Ship Staff","Ship Staff Insp.","STEAM BRANCH LINE AT HEAT EXCHANGER HEAVILY CORRODED AND BROKEN","Deck - Pipe / Fittings","General Appearance","Inappropriate Procedure","11.6","Medium","","","Corroded steam lines have been renewed at Drydock. De-Rusting and painting on corroded areas carried out.","2019-12-28","","Completed","2020-01-05","No","No","No","Internal"]
[null,null,null,null,8492,"86_Wed Oct 09 2019 09:14:11 GMT+0000 (Coordinated Universal Time)","2019-06-28","Defect","Ship Staff","Ship Staff Insp.","SOPT RUST ON STEAM BRANCH LINES THROUGHOUT THE SHIP","Deck - Pipe / Fittings","General Appearance","Inappropriate Procedure","11.6","Medium","","","De- Rusting and Painting on steam branch lines carried out. Damaged steam lines have been renewed at Dry Dock.","2019-12-28","","Completed","2020-01-10","No","No","No","Internal"]
[null,null,null,null,8493,"86_Wed Oct 09 2019 09:42:59 GMT+0000 (Coordinated Universal Time)","2019-06-28","Defect","Ship Staff","Ship Staff Insp.","FOAM LINE ,FIRE LINE STEAM LINE ,IG LINE , SPOT RUST AT THE BOTTOM OF THE PIPE THROUGHOUT THE SHIPS LENGTH, INCLUDING THE BRANCH LINE CLAMPS ARE ALSO RUSTED","Deck - Pipe / Fittings","General Appearance","Inappropriate Procedure","11.6","Medium","","","De-Rusting and painting on pipelines till midship area.","2019-12-28","","Completed","2019-12-10","No","No","No","Internal"]
[null,null,null,null,8494,"86_Tue Sep 10 2019 09:46:29 GMT+0000 (Coordinated Universal Time)","2019-06-28","Defect","Ship Staff","Ship Staff Insp.","BUNKER MANIFOLD PRESENTATION FLANGE NOT IN GOOD CONDITION","Deck - Pipe / Fittings","General Appearance","Inappropriate Procedure","","","","","FLANGE RENEWED.","2019-07-28","","Completed","2019-08-11","No","No","No","Internal"]
[null,null,null,null,8495,"86_Tue Sep 10 2019 09:51:49 GMT+0000 (Coordinated Universal Time)","2019-06-28","Defect","Ship Staff","Ship Staff Insp.","TRACES OF LEAKAGE FOUND AT ALL FOAM MONITOR SEAL","LSA / FFA","Safety / LSA / FFA","Inappropriate Procedure","5.35","Medium","","","Overhauling of Foam monitor valves carried out. Renewal of leaking gate valve carried out.","2019-07-28","","Completed","2019-12-25","No","No","No","Internal"]
[null,null,null,null,8497,"86_Wed Oct 09 2019 10:20:25 GMT+0000 (Coordinated Universal Time)","2019-06-28","Defect","Ship Staff","Ship Staff Insp.","BALLAST TANK LEVEL GAUGE SHOWING INCORRECT READINGS IN CCR","Cargo Mach.","Cargo / Ballast Systems","Inappropriate Procedure","8.8","Very High","","","Ballast tank level Sensors renewal carried out in Dry Dock ","2019-12-29","","Completed","2020-01-10","No","No","No","Internal"]
[null,null,null,null,8520,"86_Wed Oct 09 2019 09:17:56 GMT+0000 (Coordinated Universal Time)","2019-06-28","Defect","Ship Staff","Ship Staff Insp.","CONDUIT BOX AND ITS PIPES NEAR MIDSHIP STORE HEAVILY CORRODED","Deck - Pipe / Fittings","General Appearance","Inappropriate Procedure","11.6","Medium","","","DERUSTING AND PAINTING CARRIED OUT.","2019-07-28","","Completed","2019-08-13","No","No","No","Internal"]
[null,null,null,null,8521,"86_Wed Oct 09 2019 09:27:40 GMT+0000 (Coordinated Universal Time)","2019-06-28","Defect","Ship Staff","Ship Staff Insp.","NO CANVAS COVER FOR MOORINGS ROPES ON DRUM ","Deck - Mooring Machinery","Mooring","Inappropriate Procedure","9.4","High","","","CANVAS COVER FOR MOORING LINE STICHED AND COVERED ON ALL WINCHES.","2019-07-14","","Completed","2019-10-08","No","No","No","Internal"]
[null,null,null,null,8522,"86_Wed Oct 09 2019 09:54:41 GMT+0000 (Coordinated Universal Time)","2019-06-28","Defect","Ship Staff","Ship Staff Insp.","NO. 1 & NO. 2 FOAM MONITOR HARD TO OPERATE","LSA / FFA","Safety / LSA / FFA","Inappropriate Procedure","5.35","Medium","","","REMOVAL OF OLD GREASE CARRIED OUT. ALL MOVING PARTS GREASED AND MADE FREE.","2019-07-28","","Completed","2019-08-25","No","No","No","Internal"]
[null,null,null,null,8523,"86_Wed Oct 09 2019 10:07:08 GMT+0000 (Coordinated Universal Time)","2019-06-28","Defect","Ship Staff","Ship Staff Insp.","IN CCR 1 S AND 3 STBD VALVE INDICATION FOR FULL OPEN AND SHUT NOT WORKING","Deck - Machinery","Cargo / Ballast Systems","Inappropriate Procedure","8.8","Very High","","","All cargo discharge valves calibration and serivicing carried out by HYDEL Tech. at Dry Dock.","2019-07-28","","Completed","2019-07-05","No","No","No","Internal"]
[null,null,null,null,8541,"86_Wed Oct 09 2019 10:24:04 GMT+0000 (Coordinated Universal Time)","2019-06-28","Defect","Ship Staff","Ship Staff Insp.","PORT SIDE EYE WASH DRAIN VALVE NOT HOLDING","LSA / FFA","Safety / LSA / FFA","Inappropriate Procedure","","","","","EYE WASH DRAIN VALVE RENEWAL CARRIED OUT.","2019-07-29","","Completed","2019-10-20","No","No","No","Internal"]
[null,null,null,null,3058,"86_2019-10-09 09:17:56.000","2019-06-28","Defect","Ship Staff","Ship Staff Insp.","CONDUIT BOX AND ITS PIPES NEAR MIDSHIP STORE HEAVILY CORRODED","Deck - Pipe / Fittings","General Appearance","Inappropriate Procedure","11.6","Medium","","","De-Rusting and Painting carried out in Drydock ","2019-07-28","","Completed","2019-08-13","No","No","No","Internal"]
[null,null,null,null,3059,"86_2019-10-09 09:54:41.000","2019-06-28","Defect","Ship Staff","Ship Staff Insp.","NO. 1 & NO. 2 FOAM MONITOR HARD TO OPERATE","LSA / FFA","Safety / LSA / FFA","Inappropriate Procedure","5.35","Medium","","","Foam monitiors cleaned, de-rusted and all moving parts cleaned and greased. Found operational and good in order.","2019-07-28","","Completed","2019-08-25","No","No","No","Internal"]
[null,null,null,null,3060,"86_2019-10-09 09:27:40.000","2019-06-28","Defect","Ship Staff","Ship Staff Insp.","NO CANVAS COVER FOR MOORINGS ROPES ON DRUM ","Deck - Mooring Machinery","Mooring","Inappropriate Procedure","9.4","High","","","New canvas Cover for all mooring ropes stiched and same has bben covered on all winches","2019-07-14","","Completed","2019-10-08","No","No","No","Internal"]
[null,null,null,null,3061,"86_2019-10-09 10:07:08.000","2019-06-28","Defect","Ship Staff","Ship Staff Insp.","IN CCR 1 S AND 3 STBD VALVE INDICATION FOR FULL OPEN AND SHUT NOT WORKING","Deck - Machinery","Cargo / Ballast Systems","Inappropriate Procedure","8.8","Very High","","","Calibration and serivicing of VRCS system carried and problem resolved by Shore Tech. at Drydock.","2019-07-28","","Completed","2019-07-05","No","No","No","Internal"]
[null,null,null,null,3102,"86_2019-09-10 13:30:52.000","2019-06-30","Defect","Ship Staff","Ship Staff Insp.","PV VALVE TEST KIT NOT AVAILABLE ON BOARD","Cargo Mach.","Cargo / Ballast Systems","Inappropriate Procedure","8.8","Very High","","","PV VALVE TEST KIT RECEIVED IN DRY-DOCK ","2019-07-29","","Completed","2019-12-05","No","No","No","Internal"]
[null,null,null,null,3107,"86_2019-10-10 13:29:17.000","2019-06-30","Defect","Ship Staff","Ship Staff Insp.","FWD AND AFT ADDITIONAL WINCH CONTROLLER NEVER TRIED OUT BY SHIPS STAFF COVER ARE HARD ","Deck - Mooring Machinery","Mooring","Inappropriate Procedure","","","","","ADDITIONAL WINCH CONTROLLERS LEVERS OVERHAULED IN DRYDOCK. ","2019-07-29","","Completed","2020-01-07","No","No","No","Internal"]
[null,null,null,null,8498,"86_Wed Oct 09 2019 13:30:52 GMT+0000 (Coordinated Universal Time)","2019-06-30","Defect","Ship Staff","Ship Staff Insp.","PV VALVE TEST KIT NOT AVAILABLE ON BOARD","Cargo Mach.","Cargo / Ballast Systems","Inappropriate Procedure","8.8","Very High","","","PV Valve test kit received on baord at Drydock.","2019-12-29","","Completed","2019-12-05","No","No","No","Internal"]
[null,null,null,null,8503,"86_Thu Oct 10 2019 13:29:17 GMT+0000 (Coordinated Universal Time)","2019-06-30","Defect","Ship Staff","Ship Staff Insp.","FWD AND AFT ADDITIONAL WINCH CONTROLLER NEVER TRIED OUT BY SHIPS STAFF COVER ARE HARD ","Deck - Mooring Machinery","Mooring","Inappropriate Procedure","","","","","Cover of additional winch controller freed and greased","2019-12-25","","Completed","2019-12-03","No","No","No","Internal"]
[null,null,null,null,8524,"86_Wed Oct 09 2019 13:23:57 GMT+0000 (Coordinated Universal Time)","2019-06-30","Defect","Ship Staff","Ship Staff Insp.","IN CCR 3P,4P,5 PORT  CARGO DISCH VALVE FULL OPEN INDICATION NOT WORKING","Cargo Mach.","Cargo / Ballast Systems","Inappropriate Procedure","8.8","Very High","","","All cargo discharge valves calibration and serivicing carried out by HYDEL Tech. at Dry Dock.","2019-07-30","","Completed","2019-09-16","No","No","No","Internal"]
[null,null,null,null,8525,"86_Wed Oct 09 2019 13:41:45 GMT+0000 (Coordinated Universal Time)","2019-06-30","Defect","Ship Staff","Ship Staff Insp.","ALL GAS MEASURING INST. CALIBRATION EXPIRED","Cargo Mach.","Cargo / Ballast Systems","Inappropriate Procedure","5.22","High","","","NEW CALIBRATION CERTIFICATE ISSUED.","2019-07-04","","Completed","2019-07-12","No","No","No","Internal"]
[null,null,null,null,8526,"86_Wed Oct 09 2019 13:47:30 GMT+0000 (Coordinated Universal Time)","2019-06-30","Defect","Ship Staff","Ship Staff Insp.","FWD PORT SIDE LOOSE ROPE STRANDS FOUND BROKEN AT THREE PLACE","Deck - Mooring Machinery","Mooring","Inappropriate Procedure","9.8","Medium","","","NEW MOORING ROPES RECEIVED ON BOARD AND REPLACED DAMAGED ONES.","2019-07-15","","Completed","2019-07-23","No","No","No","Internal"]
[null,null,null,null,3062,"86_2019-10-09 13:23:57.000","2019-06-30","Defect","Ship Staff","Ship Staff Insp.","IN CCR 3P,4P,5 PORT  CARGO DISCH VALVE FULL OPEN INDICATION NOT WORKING","Cargo Mach.","Cargo / Ballast Systems","Inappropriate Procedure","8.8","Very High","","","All cargo discharge valves calibration and serivicing carried out by HYDEL Tech. at Dry Dock.","2019-07-30","","Completed","2019-09-16","No","No","No","Internal"]
[null,null,null,null,3063,"86_2019-10-09 13:41:45.999","2019-06-30","Defect","Ship Staff","Ship Staff Insp.","ALL GAS MEASURING INST. CALIBRATION EXPIRED","Cargo Mach.","Cargo / Ballast Systems","Inappropriate Procedure","5.22","High","","","New Calibration Certificate received for all Gas measuring instruments.","2019-07-04","","Completed","2019-07-12","No","No","No","Internal"]
[null,null,null,null,3064,"86_2019-10-09 13:47:30.000","2019-06-30","Defect","Ship Staff","Ship Staff Insp.","FWD PORT SIDE LOOSE ROPE STRANDS FOUND BROKEN AT THREE PLACE","Deck - Mooring Machinery","Mooring","Inappropriate Procedure","9.8","Medium","","","New mooring Ropes received on board and renewal of damaged ropes carried out.","2019-07-15","","Completed","2019-07-23","No","No","No","Internal"]
[null,null,null,null,3086,"86_23/10/2019 10:43:27 PM","2019-07-01","Defect","Ship Staff","Ship Staff Insp.","LIFE BOAT RR TAPE FADED","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","RR Tape renewed at Dry dock.","2019-07-15","","Completed","2019-07-20","No","No","No","Internal"]
[null,null,null,null,3108,"86_2019-10-10 13:47:41.999","2019-07-01","Defect","Ship Staff","Ship Staff Insp.","EYE WASH MAIN LINE ON MAIN DECK HEAVILY CORRODED AT SOME PLACE .","Deck - Pipe / Fittings","Safety / LSA / FFA","Inappropriate Procedure","","","","","DE-RUSTING AND PAINITING CARRIED OUT ON CORRODED AREAS  ON EYE WASH LINE. ","2019-08-01","","Completed","2020-01-08","No","No","No","Internal"]
[null,null,null,null,8504,"86_Thu Oct 10 2019 13:47:41 GMT+0000 (Coordinated Universal Time)","2019-07-01","Defect","Ship Staff","Ship Staff Insp.","EYE WASH MAIN LINE ON MAIN DECK HEAVILY CORRODED AT SOME PLACE .","Deck - Pipe / Fittings","Safety / LSA / FFA","Inappropriate Procedure","","","","","De- Rusting of Eye Wash main line at corroded areas carried out.","2019-12-08","","Completed","2019-12-15","No","No","No","Internal"]
[null,null,null,null,8528,"86_Thu Oct 10 2019 13:32:34 GMT+0000 (Coordinated Universal Time)","2019-07-01","Defect","Ship Staff","Ship Staff Insp.","CHEMICAL STOWED  ON MIDSHIP STORE FOUND LEAKINGS","Miscellaneous","MARPOL Related","Inappropriate Procedure","","","","","TRANSFERRED TO NEW DRUM","2019-07-06","","Completed","2019-07-20","No","No","No","Internal"]
[null,null,null,null,8529,"86_Thu Oct 10 2019 13:43:43 GMT+0000 (Coordinated Universal Time)","2019-07-01","Defect","Ship Staff","Ship Staff Insp.","VERTICAL SUPPORTFOR PIPELINE AT 5 PORT AT PUMP STACK HAVE HOLE DUE TO HEAVY CORROSION","Deck - Pipe / Fittings","Cargo / Ballast Systems","Inappropriate Procedure","","","","","COLD WORK CARRIED OUT FOR PERMANENT REPAIR IN DRY DOCK ","2019-08-01","","Completed","2019-09-08","No","No","No","Internal"]
[null,null,null,null,3053,"86_23/10/2019 5:05:10 PM","2019-07-01","Defect","Ship Staff","Ship Staff Insp.","BOTH LIFEBOAT INNER AND OUTER PAINT FADED","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","BOTH LIFEBOATS PAINTED IN DRYDOCK. ","2019-11-01","","Completed","2020-01-05","Yes","No","No","Internal"]
[null,null,null,null,3066,"86_2019-10-10 13:32:34.000","2019-07-01","Defect","Ship Staff","Ship Staff Insp.","CHEMICAL STOWED  ON MIDSHIP STORE FOUND LEAKINGS","Miscellaneous","MARPOL Related","Inappropriate Procedure","","","","","Chemicals have been transferred to another drum and shifted to Chemical locker.","2019-07-06","","Completed","2019-07-20","No","No","No","Internal"]
[null,null,null,null,3067,"86_2019-10-10 13:43:43.000","2019-07-01","Defect","Ship Staff","Ship Staff Insp.","VERTICAL SUPPORTFOR PIPELINE AT 5 PORT AT PUMP STACK HAVE HOLE DUE TO HEAVY CORROSION","Deck - Pipe / Fittings","Cargo / Ballast Systems","Inappropriate Procedure","","","","","De- Rusting and painting carried out at Dry dock.","2019-08-01","","Completed","2019-09-08","No","No","No","Internal"]
[null,null,null,null,3072,"86_2019-10-11 13:11:26.000","2019-07-02","Defect","Ship Staff","Ship Staff Insp.","SPARE PIPE ON FUNNEL DECK NOT PROPERLY SECURED","Miscellaneous","General Appearance","Inappropriate Procedure","","","","","All Pipelines lashed and secured properly on deck.","2019-07-15","","Completed","2019-08-16","No","No","No","Internal"]
[null,null,null,null,3087,"86_23/10/2019 10:52:31 PM","2019-07-02","Defect","Ship Staff","Ship Staff Insp.","LIFE BOAT AND LIFE RAFT EMBARKATION POSTER NOT PASTED UNDER THE EMERGENCY LIGHT","LSA / FFA","Safety / LSA / FFA","Inappropriate Procedure","","","","","LIFE BOAT AND LIFE RAFT EMBARKATION POSTER PASTED UNDER THE EMERGENCY LIGHT. ","2019-07-15","","Completed","2019-08-15","No","No","No","Internal"]
[null,null,null,null,3088,"86_23/10/2019 10:59:11 PM","2019-07-02","Defect","Ship Staff","Ship Staff Insp.","FOAM ROOM EEBD FOUND AT LOW PRESSURE. ADAPTER NOT AVAILABLE ONBOARD FOR REFILLING","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","ANNUAL SERVICING AND REPAIR OF EEBD CARRIED OUT IN DRYDOCK.","2019-07-15","","Completed","2019-08-09","No","No","No","Internal"]
[null,null,null,null,3089,"86_23/10/2019 11:05:02 PM","2019-07-02","Defect","Ship Staff","Ship Staff Insp.","FIREMAN OUTFIT BOX IS NOT AVAILABLE FOR ONE FIREMAN OUTFIT ON BRIDGE DECK. PRESENTLY IT HAS BEEN KEPT OUT OF BOX","LSA / FFA","Safety / LSA / FFA","Inappropriate Procedure","","","","","NEW FIREMEN OUTFIT FABRICATED AND PLACED ON FIRE LOCKER.","2019-07-30","","Completed","2019-08-03","No","No","No","Internal"]
[null,null,null,null,3109,"86_2019-10-10 15:33:02.000","2019-07-02","Defect","Ship Staff","Ship Staff Insp.","GRACO PUMP NOT AVAILABLE ON BOARD","Deck - Machinery","Cargo / Ballast Systems","Inappropriate Procedure","","","","","VESSEL DOESN'T REQUIRE GRACO PUMP PRESENTLY AS IT CARRIES PRODUCTS ONLY.","2019-07-30","","Completed","2019-12-02","No","No","No","Internal"]
[null,null,null,null,3110,"86_2019-10-10 15:35:29.000","2019-07-02","Defect","Ship Staff","Ship Staff Insp.","VALVE WHEEL FOR ODME FRESH WATER FLUSHING LINE BROKEN","Deck - Machinery","Cargo / Ballast Systems","Inappropriate Procedure","","","","","NEW VALVE WHEEL FOR ODME FRESH WATER HAS BEEN INSTALLED AND FOUND OPERATIONAL","2019-07-15","","Completed","2019-08-05","No","No","No","Internal"]
[null,null,null,null,3111,"86_2019-11-10 13:08:12.999","2019-07-02","Defect","Ship Staff","Ship Staff Insp.","CCTV CAMERA ON BRIDGEWING NOT WORKING ","Accommodation","General Appearance","Inappropriate Procedure","","","","","CCTV CAMERA ON BRIDGE WINGS HAVE BEEN REMOVED.","2019-07-30","","Completed","2019-08-20","No","No","No","Internal"]
[null,null,null,null,3112,"86_2019-10-11 13:15:32.000","2019-07-02","Defect","Ship Staff","Ship Staff Insp.","OFFICER AND CREW SMOKE ROOM CUP BOARD DOOR BROKEN ","Accommodation","General Appearance","Inappropriate Procedure","","","","","BROKEN DOOR HAS BEEN REPAIRED.","2019-07-15","","Completed","2019-07-22","No","No","No","Internal"]
[null,null,null,null,3113,"86_2019-10-11 13:18:36.000","2019-07-02","Defect","Ship Staff","Ship Staff Insp.","MARKING AT  PUMPSTACK , ULLAGE POCKETS SOUNDING PIPES MISSING","Deck - Machinery","Cargo / Ballast Systems","Inappropriate Procedure","","","","","MARKING AT  PUMPSTACK , ULLAGE POCKETS SOUNDING PIPES CARRIED OUT ","2019-07-15","","Completed","2019-09-20","No","No","No","Internal"]
[null,null,null,null,3120,"86_23/10/2019 11:54:43 PM","2019-07-02","Defect","Ship Staff","Ship Staff Insp.","IMO SYMOLS MISSING AT VARIOUS EMERGENCY EQUIPMENTS AND PLACES","LSA / FFA","Safety / LSA / FFA","Equipment Related,External Factors","","","","","ALL IMO SYMBOLS HAVE PUT IN PLACE AND FADED ONES HAVE BEEN REPLACED.","2019-07-15","VIRG195025","Completed","2019-08-10","No","No","No","Internal"]
[null,null,null,null,8505,"86_Thu Oct 10 2019 15:33:02 GMT+0000 (Coordinated Universal Time)","2019-07-02","Defect","Ship Staff","Ship Staff Insp.","GRACO PUMP NOT AVAILABLE ON BOARD","Deck - Machinery","Cargo / Ballast Systems","Inappropriate Procedure","","","","","Vessel doesn't require Graco Pump presently as it carries Products presently.","2019-12-21","","Completed","2019-12-01","No","No","No","Internal"]
[null,null,null,null,8506,"86_Fri Oct 11 2019 13:08:12 GMT+0000 (Coordinated Universal Time)","2019-07-02","Defect","Ship Staff","Ship Staff Insp.","CCTV CAMERA ON BRIDGEWING NOT WORKING ","Accommodation","General Appearance","Inappropriate Procedure","","","","","CCTV camera founf not operational and removed from the Bridge wing.","2019-12-30","","Completed","2019-08-15","No","No","No","Internal"]
[null,null,null,null,8530,"86_Thu Oct 10 2019 13:50:19 GMT+0000 (Coordinated Universal Time)","2019-07-02","Defect","Ship Staff","Ship Staff Insp.","2P COT DISCHARGE LINE DRAIN VALVE LEAKING","Cargo Mach.","Cargo / Ballast Systems","Inappropriate Procedure","","","","","LEAKING DRAIN VALVE RENEWED.","2019-07-03","","Completed","2019-07-03","No","No","No","Internal"]
[null,null,null,null,8531,"86_Thu Oct 10 2019 15:37:56 GMT+0000 (Coordinated Universal Time)","2019-07-02","Defect","Ship Staff","Ship Staff Insp.","4S & SLOP PORT PUMPSTACK PRESSURE GAUGE BROKEN ","Cargo Mach.","Cargo / Ballast Systems","Inappropriate Procedure","","","","","NEW PRESSURE GUAGES INSTALLED ON PUMPSTACK.","2019-07-02","","Completed","2019-07-21","No","No","No","Internal"]
[null,null,null,null,8534,"86_Fri Oct 11 2019 13:11:26 GMT+0000 (Coordinated Universal Time)","2019-07-02","Defect","Ship Staff","Ship Staff Insp.","SPARE PIPE ON FUNNEL DECK NOT PROPERLY SECURED","Miscellaneous","General Appearance","Inappropriate Procedure","","","","","SECURING TO BE CARRIED OUT UPON TAKEOVER","2019-07-15","","Completed","2019-08-16","No","No","No","Internal"]
[null,null,null,null,8542,"86_Sun Nov 10 2019 13:15:32 GMT+0000 (Coordinated Universal Time)","2019-07-02","Defect","Ship Staff","Ship Staff Insp.","OFFICER AND CREW SMOKE ROOM CUP BOARD DOOR BROKEN ","Accommodation","General Appearance","Inappropriate Procedure","","","","","DOOR HAS BEEN REPAIRED AND FIXED BACK IN PLACE.","2019-07-15","","Completed","2019-10-20","No","No","No","Internal"]
[null,null,null,null,8543,"86_Thu Oct 10 2019 15:35:29 GMT+0000 (Coordinated Universal Time)","2019-07-02","Defect","Ship Staff","Ship Staff Insp.","VALVE WHEEL FOR ODME FRESH WATER FLUSHING LINE BROKEN","Deck - Machinery","Cargo / Ballast Systems","Inappropriate Procedure","","","","","WHEEL VALVE HAS BEEN RENEWED AND FOUND OPERATIONAL.","2019-07-15","","Completed","2019-11-15","No","No","No","Internal"]
[null,null,null,null,8544,"86_Sun Nov 10 2019 13:18:36 GMT+0000 (Coordinated Universal Time)","2019-07-02","Defect","Ship Staff","Ship Staff Insp.","MARKING AT  PUMPSTACK , ULLAGE POCKETS SOUNDING PIPES MISSING","Deck - Machinery","Cargo / Ballast Systems","Inappropriate Procedure","","","","","STENCILLING ON PUMPSTACK , ULLAGE POCKETS SOUNDING PIPES  CARRIED OUT ","2019-07-15","","Completed","2019-10-14","No","No","No","Internal"]
[null,null,null,null,3054,"86_23/10/2019 5:08:39 PM","2019-07-02","Defect","Ship Staff","Ship Staff Insp.","NO DEDICATED WALKIE TALKIE FOR FIREMAN OUTFIT","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","DEDICATED WALKIE TALKIES FOR FIREFIGHTING HAS BEEN SUPPLIED ","2019-07-15","","Completed","2020-01-12","No","No","No","Internal"]
[null,null,null,null,3068,"86_2019-10-10 13:50:19.999","2019-07-02","Defect","Ship Staff","Ship Staff Insp.","2P COT DISCHARGE LINE DRAIN VALVE LEAKING","Cargo Mach.","Cargo / Ballast Systems","Inappropriate Procedure","","","","","Drain valve changed and leakge stopped.","2019-07-03","","Completed","2019-07-03","No","No","No","Internal"]
[null,null,null,null,3069,"86_2019-10-10 15:37:56.999","2019-07-02","Defect","Ship Staff","Ship Staff Insp.","4S & SLOP PORT PUMPSTACK PRESSURE GAUGE BROKEN ","Cargo Mach.","Cargo / Ballast Systems","Inappropriate Procedure","","","","","Pumpstack RPM Guage renewed by new one and found operational.","2019-07-02","","Completed","2019-07-21","No","No","No","Internal"]
[null,null,null,null,3073,"86_2019-10-11 13:28:56.999","2019-07-03","Defect","Ship Staff","Ship Staff Insp.","WALK WAY PLATFORM NEAR STBD SIDE GANGWAY LOOSELY FITTED","Miscellaneous","General Appearance","Inappropriate Procedure","","","","","All Walkway platform de- rusted and painting carried out. Damaged ones were fabricated on board.","2019-07-15","","Completed","2019-08-24","No","No","No","Internal"]
[null,null,null,null,3114,"86_2019-11-10 13:23:17.000","2019-07-03","Defect","Ship Staff","Ship Staff Insp.","SIGHTING PORT ON EEBD COVER TO CHECK THE LEVEL OF PRESSURE IS DAMAGE AT FEW LOCATION IN ACCCOMODATION AND ALMOST FOR ALL IN ER. ","LSA / FFA","Safety / LSA / FFA","Inappropriate Procedure","","","","","ANNAUL SERIVICING OF EEBD CARRIED OUT IN DRYDOCK. DAMAGED PARTS REPLACED.","2019-07-15","","Completed","2019-12-29","No","No","No","Internal"]
[null,null,null,null,3115,"86_2019-11-10 13:25:43.999","2019-07-03","Defect","Ship Staff","Ship Staff Insp.","THE SENSOR LOCATION STENCILLED IN ACCOMODATION ARE FADED","Accommodation","Safety / LSA / FFA","Inappropriate Procedure","","","","","STENCILLING AND MARKING ON SENSOR LOCATIONS CARRIED OUT. ","2019-07-15","","Completed","2019-09-20","No","No","No","Internal"]
[null,null,null,null,3116,"86_2019-11-10 13:32:49.000","2019-07-03","Defect","Ship Staff","Ship Staff Insp.","4X200L METAL DRUM ON EACH SIDE FOR ANTIPOLLUTION ARE CORRODED AND CAPS MISSING.","Cargo Mach.","MARPOL Related","Inappropriate Procedure","","","","","NEW PLASTIC SOPEP DRUMS RECEIVED AND REPLACED THE OLD CORRODED ONES.","2019-07-30","","Completed","2019-07-26","No","No","No","Internal"]
[null,null,null,null,8507,"86_Sun Nov 10 2019 13:23:17 GMT+0000 (Coordinated Universal Time)","2019-07-03","Defect","Ship Staff","Ship Staff Insp.","SIGHTING PORT ON EEBD COVER TO CHECK THE LEVEL OF PRESSURE IS DAMAGE AT FEW LOCATION IN ACCCOMODATION AND ALMOST FOR ALL IN ER. ","LSA / FFA","Safety / LSA / FFA","Inappropriate Procedure","","","","","Sighting Port of EEBD Cover repaired and annual servicing of EEBD carried out at Dry Dock.","2019-07-15","","Completed","2020-12-29","No","No","No","Internal"]
[null,null,null,null,8508,"86_Sun Nov 10 2019 13:25:43 GMT+0000 (Coordinated Universal Time)","2019-07-03","Defect","Ship Staff","Ship Staff Insp.","THE SENSOR LOCATION STENCILLED IN ACCOMODATION ARE FADED","Accommodation","Safety / LSA / FFA","Inappropriate Procedure","","","","","STENCILLING CARRIED OUT ON SENSOR LOCATIONS AND VARIOUS LOCATIONS","2019-07-15","","Completed","2019-08-25","No","No","No","Internal"]
[null,null,null,null,8509,"86_Fri Oct 11 2019 13:32:49 GMT+0000 (Coordinated Universal Time)","2019-07-03","Defect","Ship Staff","Ship Staff Insp.","4X200L METAL DRUM ON EACH SIDE FOR ANTIPOLLUTION ARE CORRODED AND CAPS MISSING.","Cargo Mach.","MARPOL Related","Inappropriate Procedure","","","","","NEW PLASTIC SOPEP DRUMS RECEIVED ON BOARD AND REPLACED OLD CORRODED ONES","2019-12-30","","Completed","2019-07-25","No","No","No","Internal"]
[null,null,null,null,8535,"86_Fri Oct 11 2019 13:28:56 GMT+0000 (Coordinated Universal Time)","2019-07-03","Defect","Ship Staff","Ship Staff Insp.","WALK WAY PLATFORM NEAR STBD SIDE GANGWAY LOOSELY FITTED","Miscellaneous","General Appearance","Inappropriate Procedure","","","","","NEED TO TIGHTNED NEW NUT BOLT UPON TAKE OVER","2019-07-15","","Completed","2019-08-24","No","No","No","Internal"]
[null,null,null,null,3055,"86_23/10/2019 5:13:36 PM","2019-07-03","Defect","Ship Staff","Ship Staff Insp.","SIGHTING PORT OF EEBD TO CHECK. THE LEVEL OF PRESSURE IS DAMAGED IN FEW LOCATIONS AT ACCOM. AND ALMOST ALL IN E/R","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","SERVICING OF EEBD CARRIED OUT IN DRYDOCK. ALL EEBD ARE IN GOOD CONDITION AND NO SIGNS OF DAMAGE","2019-07-15","","Completed","2020-01-03","No","No","No","Internal"]
[null,null,null,null,3090,"86_23/10/2019 11:12:19 PM","2019-07-04","Non Conformity","Ship Staff","Ship Staff Insp.","BA COMPRESSOR NOT IN WORKING CONDITION","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","NEW BA COMPRESSOR RECEIVED AND OPERATIONAL ON BOARD.","2019-07-15","VIRG195058","Completed","2019-07-23","No","No","No","Internal"]
[null,null,null,null,3091,"86_23/10/2019 11:28:56 PM","2019-07-04","Non Conformity","Ship Staff","Ship Staff Insp.","AIR QUALITY CERTIFICATE EXPIRED","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","NEW AIR QUALITY CHECK CERTIFICATE RECEIVED WITH THE NEW BA COMPRESSOR","2019-07-15","VIRG195058","Completed","2019-07-23","No","No","No","Internal"]
[null,null,null,null,3092,"86_23/10/2019 11:39:06 PM","2019-07-04","Non Conformity","Ship Staff","Ship Staff Insp.","AS PER CERTIFICATE TOTAL 4 RECISUSITATOR BOTTLE AVILABLE ONBOARD BUT ONLY THREE SIGHTED AND ONE IS MISSING","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","PROBLEM RESOLVED AND FOUR RECISUSITATOR FOUND ON BOARD.,","2019-07-15","","Completed","2019-08-21","No","No","No","Internal"]
[null,null,null,null,3056,"86_23/10/2019 5:16:48 PM","2019-07-04","Non Conformity","Ship Staff","Ship Staff Insp.","ONE RECISUSITATOR BOTTLE CONNECTION TO MASK BROKEN. TEMPORARILY REPAIRED","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","CONNECTION RENEWED AND SERVICING CARRIED OUT IN DRYDOCK ","2019-07-15","","Completed","2019-12-25","No","No","No","Internal"]
[null,null,null,null,3076,"86_23/10/2019 7:55:11 AM","2019-07-10","Defect","Ship Staff","Ship Staff Insp.","MAIN ENGINE  PRE HEAT STEAM INLET VALVE FOUND LEAKING","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","REMOVED AND  RENEWED THE VALVE","2019-07-30","","Completed","2019-07-14","No","No","No","Internal"]
[null,null,null,null,3077,"86_23/10/2019 9:12:47 AM","2019-07-11","Defect","Ship Staff","Ship Staff Insp.","2(STBD) DIESOL OIL BUNKER TANK QUICK CLOSING VALVE WAS NOT OPERATONG CORRECTLY","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","REMOVED FROM PLACE AND OVERHAULED","2019-07-30","","Completed","2019-07-14","No","No","No","Internal"]
[null,null,null,null,3103,"86_2019-10-10 09:45:42.999","2019-07-11","Breakdown","Ship Staff","Ship Staff Insp.","BILGE PUMP RELIEF VALVE SPRING BROKEN","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","SPARES RECEIVED, LINE FABRICATED AND SPRING RENEWED.","2019-11-30","VIRG190031","Completed","2019-08-15","No","No","No","Internal"]
[null,null,null,null,8499,"86_Thu Oct 10 2019 09:45:42 GMT+0000 (Coordinated Universal Time)","2019-07-11","Breakdown","Ship Staff","Ship Staff Insp.","BILGE PUMP RELIEF VALVE SPRING BROKEN","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","relief valve renewed.","2019-11-30","VIRG190031","Completed","2019-08-15","No","No","No","Internal"]
[null,null,null,null,8527,"86_Thu Oct 10 2019 10:27:00 GMT+0000 (Coordinated Universal Time)","2019-07-11","Defect","Ship Staff","Ship Staff Insp.","SEWAGE PLANT EDUCTOR PUMP TAKING MORE TIME TO BUILD UP THE VACUUM","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","EDUCTOR NOZZLE CLEANED AND NRV VALVE REPLACED WITH NEW ONE. PUMP ALSO CHECKED FOR ANY OBSTRUCTION AT THE IMPELLER EYE","2019-08-10","","Completed","2019-08-05","No","No","No","Internal"]
[null,null,null,null,3065,"86_2019-10-10 10:27:00.000","2019-07-11","Defect","Ship Staff","Ship Staff Insp.","SEWAGE PLANT EDUCTOR PUMP TAKING MORE TIME TO BUILD UP THE VACUUM","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","EDUCTOR NOZZLE CLEANED AND NRV VALVE REPLACED WITH NEW ONE. PUMP ALSO CHECKED FOR ANY OBSTRUCTION AT THE IMPELLER EYE","2019-08-10","","Completed","2019-08-05","No","No","No","Internal"]
[null,null,null,null,3075,"86_23/10/2019 7:46:51 AM","2019-07-15","Defect","Ship Staff","Ship Staff Insp.","L.T COOLER #2 SEA WATER SIDE INLET AND OUTLET VALVES WERE FOUND NOT HOLDING","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","L.T COOLER #2 ISOLATED, REMOVED AND REPLACED BOTH THE SEA WATER SIDE INLET AND OUTLET VALVES","2019-07-25","","Completed","2019-07-15","No","No","No","Internal"]
[null,null,null,null,3083,"86_23/10/2019 9:53:31 AM","2019-07-15","Defect","Ship Staff","Ship Staff Insp.","BOILER DOSING PUMP NOT OPERATIONAL","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","CHECKED AND MADE OPERATIONAL","2019-07-31","","Completed","2019-07-21","No","No","No","Internal"]
[null,null,null,null,3104,"86_2019-10-10 09:55:09.000","2019-07-18","Defect","Ship Staff","Ship Staff Insp.","THE PHONE BELL IN STEERING GEAR ROOM AND EMERGENCY GENERATOR ROOM IS NOT WORKING","Critical Equip.,Miscellaneous","Communication","Equipment Related","","","","","RECITIFIED DURING DRYDOCK AND FOUND OPERATIONAL","2019-11-30","VIRG190025","Completed","2019-08-20","No","No","No","Internal"]
[null,null,null,null,8500,"86_Thu Oct 10 2019 09:55:09 GMT+0000 (Coordinated Universal Time)","2019-07-18","Defect","Ship Staff","Ship Staff Insp.","THE PHONE BELL IN STEERING GEAR ROOM AND EMERGENCY GENERATOR ROOM IS NOT WORKING","Critical Equip.,Miscellaneous","Communication","Equipment Related","","","","","rectified.","2019-11-30","VIRG190025","Completed","2019-08-07","No","No","No","Internal"]
[null,null,null,null,8532,"86_Fri Oct 11 2019 10:17:41 GMT+0000 (Coordinated Universal Time)","2019-07-18","Breakdown","Ship Staff","Ship Staff Insp.","ME FUEL LINE SHOCK ABSORBER LEAKING INTERNALLY","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","SHOCK ABSORBER OVERHAULED WITH NEW SEAL RING. NOW FOUND NO LEAKAGE.","2019-07-30","","Completed","2019-07-24","No","No","No","Internal"]
[null,null,null,null,8533,"86_Fri Oct 11 2019 10:30:53 GMT+0000 (Coordinated Universal Time)","2019-07-18","Defect","Ship Staff","Ship Staff Insp.","ME FUEL VALVE NO.3 AND NO.4 LEAKING","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","FUEL VALVE IS REPLACED WITH OVERHAULED ONE. ","2019-07-30","","Completed","2019-07-24","No","No","No","Internal"]
[null,null,null,null,8546,"86_Wed Dec 11 2019 21:05:25 GMT+0000 (Coordinated Universal Time)","2019-07-18","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Fire hose boxes to be cleaned and spare rubber washer to be inserted in it","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","HOSE BOXES CHECKED AND ALL SPARE RUBBER WASHER PLACED IN ALL BOXES.","2019-08-20","","Completed","2019-07-28","No","No","No","Internal"]
[null,null,null,null,8549,"86_Wed Dec 11 2019 21:19:59 GMT+0000 (Coordinated Universal Time)","2019-07-18","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Inspection tags for fire extinguisher in acetylene room, Air con room, No-22 engine room bottom platform (Stbd side), No-30 in funnel near exhaust gas heater and No-29 top of IG scrubber","LSA / FFA","Safety / LSA / FFA","Inappropriate Procedure","","","","","INSPECTION TAGS CHECKED FOR ALL EXTINGUISHERS AND NEW TAGS HAVE BEEN PLACED","2019-08-22","","Completed","2019-07-29","No","No","No","Internal"]
[null,null,null,null,8566,"86_Thu Dec 12 2019 00:29:28 GMT+0000 (Coordinated Universal Time)","2019-07-18","Defect","Owner / Marine / Tech. Suptd.,Ship Staff","Suptd. Insp.","Fire plan IMO symbol to be replace at manifold (burning ship)","LSA / FFA","Safety / LSA / FFA","External Factors","","","","","NEW IMO SYMBOL REQUISITION RAISED AND OLD SYMBOLS HAVE BEEN REPLACED WITH NEW ONES","2019-08-10","VIRG195025","Completed","2019-08-05","No","No","No","Internal"]
[null,null,null,null,8574,"86_Thu Dec 12 2019 16:58:29 GMT+0000 (Coordinated Universal Time)","2019-07-18","Defect","Owner / Marine / Tech. Suptd.,Ship Staff","Suptd. Insp.","Isolation valve’s in foam room are hard to turn ","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","ISOLATION VALVE IN FOAM ROOM OVERHAULED AND MADE FREE.","2019-08-15","","Completed","2019-08-05","No","No","No","Internal"]
[null,null,null,null,8581,"86_Thu Dec 12 2019 17:45:57 GMT+0000 (Coordinated Universal Time)","2019-07-18","Defect","Owner / Marine / Tech. Suptd.,Ship Staff","Suptd. Insp.","Foundation bolts for both lifeboat to be de-rusted and painted ","LSA / FFA","Safety / LSA / FFA","External Factors,Human Error","","","","","Bolts have been de-rusted and painted. Found in Good order.","2019-08-10","","Completed","2019-08-08","No","No","No","Internal"]
[null,null,null,null,3070,"86_2019-10-11 10:17:41.999","2019-07-18","Breakdown","Ship Staff","Ship Staff Insp.","ME FUEL LINE SHOCK ABSORBER LEAKING INTERNALLY","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","SHOCK ABSORBER OVERHAULED WITH NEW SEAL RING. NOW FOUND NO LEAKAGE.","2019-07-30","","Completed","2019-07-24","No","No","No","Internal"]
[null,null,null,null,3071,"86_2019-10-11 10:30:53.000","2019-07-18","Defect","Ship Staff","Ship Staff Insp.","ME FUEL VALVE NO.3 AND NO.4 LEAKING","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","FUEL VALVE IS REPLACED WITH OVERHAULED ONE. ","2019-07-30","","Completed","2019-07-24","No","No","No","Internal"]
[null,null,null,null,8489,"86_Tue Nov 12 2019 22:32:11 GMT+0000 (Coordinated Universal Time)","2019-07-19","Defect","Owner / Marine / Tech. Suptd.,Ship Staff","Suptd. Insp.","MSDS for samples in sample locker to be verified","Miscellaneous","Cert. & Docu.","External Factors,Human Error","","","","","MSDS FOR ALL SAMPLES IN THE SAMPLE LOCKER CHECKED AND FILED IN A SEPERATE FILE.","2019-08-15","","Completed","2019-08-21","No","No","No","Internal"]
[null,null,null,null,8517,"86_Thu Dec 12 2019 17:49:53 GMT+0000 (Coordinated Universal Time)","2019-07-19","Defect","Owner / Marine / Tech. Suptd.,Ship Staff","Suptd. Insp.","Ballast tank radar remote level gauge erratic","Cargo Mach.,Elect. Mach. & Equip.","Cargo / Ballast Systems","Equipment Related,External Factors","","","","","BALLAST TANK LEVEL SENSORS RENEWED AT DRY DOCK.","2019-12-29","","Completed","2020-01-10","No","No","No","Internal"]
[null,null,null,null,8547,"86_Wed Dec 11 2019 21:11:53 GMT+0000 (Coordinated Universal Time)","2019-07-19","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Inspection records and tags for loose lifting appliances like chain blocks, wire slings, web slings and portable ladders on deck (GSM form-Record of lifting gear)","Deck - Machinery","ISM Related","Inappropriate Procedure","","","","","INSPECTION CARRIED OUT AND ALL LOOSE LIFTING APPLIANCES TAGGED","2019-08-15","","Completed","2019-08-10","No","No","No","Internal"]
[null,null,null,null,8551,"86_Wed Dec 11 2019 21:45:47 GMT+0000 (Coordinated Universal Time)","2019-07-19","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Vent for S/G blower has become hard and needs to be freed","Deck - Machinery","Eng. / Strg. Comp.","Equipment Related","","","","","VENT MADE FREED AND CHECKED FOR OPERATIO. FOUND SATISFACTORY.","2019-08-20","","Completed","2019-08-15","No","No","No","Internal"]
[null,null,null,null,8552,"86_Wed Dec 11 2019 21:50:44 GMT+0000 (Coordinated Universal Time)","2019-07-19","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Hole in deflection plate for Stbd fw tank, LO AVP, MDO AVP vent near stbd side of upper deck","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","","","","","DEFLECTION PLATE FABRICATED AND FIXED BACK IN RESPECTIVE VENTS.","2019-08-30","","Completed","2019-08-16","No","No","No","Internal"]
[null,null,null,null,8553,"86_Wed Dec 11 2019 21:54:52 GMT+0000 (Coordinated Universal Time)","2019-07-19","Defect,Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","FW sounding pipes to be fitted with security seals","Miscellaneous","Cargo / Ballast Systems","Inappropriate Procedure","","","","","FW SOUNDING PIPES SEALED WITH UNIQUE SECURITY SEAL NUMBER ON BOTH PORT AND STBD FW TANKS.","2019-07-29","","Completed","2019-07-22","No","No","No","Internal"]
[null,null,null,null,8554,"86_Wed Dec 11 2019 21:59:00 GMT+0000 (Coordinated Universal Time)","2019-07-19","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","MSDS for various paints in paint locker","Documentation","Cert. & Docu.","Inappropriate Procedure","","","","","PAINT LOCKER INVENTORY CHECKED AND MSDS UPADTED AS PER THE INVENTORY.","2019-07-27","","Completed","2019-07-21","No","No","No","Internal"]
[null,null,null,null,8555,"86_Tue Nov 12 2019 22:04:15 GMT+0000 (Coordinated Universal Time)","2019-07-19","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Clean SOPEP drums and container from inside","Miscellaneous","Cargo / Ballast Systems","Equipment Related","","","","","NEW SOPEP DRUMS ORDERED AND REPLACED OLD DRUMS.","2019-08-27","VIRG195072","Completed","2019-08-05","No","No","No","Internal"]
[null,null,null,null,8556,"86_Wed Dec 11 2019 22:14:28 GMT+0000 (Coordinated Universal Time)","2019-07-19","Defect","Owner / Marine / Tech. Suptd.,Ship Staff","Suptd. Insp.","Locking plate spring action not working for davits forward of accommodation","Deck - Machinery","ISM Related","Equipment Related","","","","","LOCKING PLATE OVERHAULED AND SPRING ACTION CHECKED. FOUND IN GOOD ORDER.","2019-08-15","","Completed","2019-08-10","No","No","No","Internal"]
[null,null,null,null,8558,"86_Wed Dec 11 2019 22:27:54 GMT+0000 (Coordinated Universal Time)","2019-07-19","Defect","Owner / Marine / Tech. Suptd.,Ship Staff","Suptd. Insp.","Glycol for ballast pumps header tanks to be topped up","Deck - Machinery","Cargo / Ballast Systems","Human Error,Inappropriate Procedure","","","","","GLYCOL FOR BOTH BALLAST PUMPS CHECKED AND TOPPED UP.","2019-08-15","","Completed","2019-08-08","No","No","No","Internal"]
[null,null,null,null,8562,"86_Wed Dec 11 2019 23:30:58 GMT+0000 (Coordinated Universal Time)","2019-07-19","Defect","Owner / Marine / Tech. Suptd.,Ship Staff","Suptd. Insp.","Inventory of sopep equipment to be updated in SMPEP and posted on location","Miscellaneous","Cert. & Docu.","External Factors,Inappropriate Procedure","","","","","ALL SOPEP EQUIPMENT INVENTORY UPDATED AND POSTED IN LOCATIONS","2019-08-10","","Completed","2019-07-28","No","No","No","Internal"]
[null,null,null,null,8563,"86_Wed Dec 11 2019 23:35:26 GMT+0000 (Coordinated Universal Time)","2019-07-19","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","MSDS for Seacare OSD to be posted in forward store","Miscellaneous","Cert. & Docu.","External Factors,Human Error","","","","","MSDS FOR SEACARE OSD POSTED IN FWD. STORE","2019-07-25","","Completed","2019-07-22","No","No","No","Internal"]
[null,null,null,null,8567,"86_Thu Dec 12 2019 00:33:24 GMT+0000 (Coordinated Universal Time)","2019-07-19","Defect","Owner / Marine / Tech. Suptd.,Ship Staff","Suptd. Insp.","IMO symbols for fire / foam valves","LSA / FFA","Safety / LSA / FFA","External Factors,Human Error","","","","","NEW IMO SYMBOLS HAVE BEEN PLACED ON ALL FIRE AND FOAM VALVES","2019-08-23","VIRG195025","Completed","2019-08-15","No","No","No","Internal"]
[null,null,null,null,8571,"86_Thu Dec 12 2019 16:42:02 GMT+0000 (Coordinated Universal Time)","2019-07-19","Defect","Owner / Marine / Tech. Suptd.,Ship Staff","Suptd. Insp.","Incorrect indication light displaying for slop equalizing valve (CO021) on CCR panel ","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","LIGHT FOR VALVE (CO021) WAS REPLACED BY NEW ONE ","2019-09-15","","Completed","2019-08-25","No","No","No","Internal"]
[null,null,null,null,8573,"86_Thu Dec 12 2019 16:55:30 GMT+0000 (Coordinated Universal Time)","2019-07-19","Other","Owner / Marine / Tech. Suptd.,Ship Staff","Suptd. Insp.","Detailed vessel particulars to be completed (form no-22.01.09.002.00) as per convenience ","Documentation","Cert. & Docu.","External Factors","","","","","NEW SHIP'S PARTICULAR COMPLETED AS PER FORM NO. -22.01.09.002.00 ","2019-08-10","","Completed","2019-08-05","No","No","No","Internal"]
[null,null,null,null,8580,"86_Thu Dec 12 2019 17:42:02 GMT+0000 (Coordinated Universal Time)","2019-07-19","Defect","Owner / Marine / Tech. Suptd.,Ship Staff","Suptd. Insp.","Torch battery for Lifeboat expired ","LSA / FFA","Safety / LSA / FFA","Equipment Related,External Factors,Human Error","","","","","Old Batteries of the torch battery was replaced by new ones and checked for its condition, found in good condition.","2019-08-10","","Completed","2019-08-06","No","No","No","Internal"]
[null,null,null,null,8582,"86_Thu Dec 12 2019 17:53:55 GMT+0000 (Coordinated Universal Time)","2019-07-19","Defect","Owner / Marine / Tech. Suptd.,Ship Staff","Suptd. Insp.","Engine cover hinge on Stbd. Life Boat  broken ","LSA / FFA","Safety / LSA / FFA","Equipment Related,External Factors","","","","","New hinges has been renewed and repaired.,","2019-08-30","","Completed","2019-08-22","No","No","No","Internal"]
[null,null,null,null,8548,"86_Wed Dec 11 2019 21:16:36 GMT+0000 (Coordinated Universal Time)","2019-07-20","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Nuts & Bolts for ISPS securing of various doors to be freed","Deck - Pipe / Fittings","ISPS Related","Equipment Related","","","","","ALL NUTS & BOLTS OF DOORS WERE FREED FOR SECURING ARRANGEMENT","2019-08-15","","Completed","2019-08-10","No","No","No","Internal"]
[null,null,null,null,8557,"86_Wed Dec 11 2019 22:19:03 GMT+0000 (Coordinated Universal Time)","2019-07-20","Defect","Owner / Marine / Tech. Suptd.,Ship Staff","Suptd. Insp.","Aft crane is observed to be entangled","Deck - Machinery","ISM Related","Equipment Related","","","","","ENTANGLED PART WAS REMOVED AND FOUND TO BE DAMGED.DAMAGED PART WAS CROPPED AND CHECKED THE CRANE OPERATION. FOUND IN GOOD ORDER.","2019-08-28","VIRG190083","Completed","2019-08-25","No","No","No","Internal"]
[null,null,null,null,8559,"86_Wed Dec 11 2019 22:36:41 GMT+0000 (Coordinated Universal Time)","2019-07-20","Defect","Owner / Marine / Tech. Suptd.,Ship Staff","Suptd. Insp.","Squaring up and securing of stores","Accommodation ,Miscellaneous","Crew Management","External Factors,Inappropriate Procedure","","","","","ALL STORES ARRANGED AND SECURED. INVENTORY OF ALL STORES TAKEN AND UPDATED","2019-08-30","","Completed","2019-08-20","No","No","No","Internal"]
[null,null,null,null,8560,"86_Wed Dec 11 2019 22:40:11 GMT+0000 (Coordinated Universal Time)","2019-07-20","Defect","Owner / Marine / Tech. Suptd.,Ship Staff","Suptd. Insp.","IMO symbol for liferaft embarkation ladder on port side missing","LSA / FFA","Safety / LSA / FFA","External Factors","","","","","IMO SYMBOLS ORDERED AND MISSING IMO SYMBOLS HAVE BEEN REPLACED WITH NEW ONES.","2019-08-30","VIRG195025","Completed","2019-08-23","No","No","No","Internal"]
[null,null,null,null,8561,"86_Wed Dec 11 2019 22:45:18 GMT+0000 (Coordinated Universal Time)","2019-07-20","Defect","Owner / Marine / Tech. Suptd.,Ship Staff","Suptd. Insp.","1 nos securing clip for fwd immersion suit box broken","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","NEW CLIP FOR THE IMMERSION SUIT BOX FABRICATED AND NEW PAINT APPLIED ON THE BOX","2019-08-08","","Completed","2019-08-02","No","No","No","Internal"]
[null,null,null,null,8564,"86_Wed Dec 11 2019 23:39:05 GMT+0000 (Coordinated Universal Time)","2019-07-20","Defect","Owner / Marine / Tech. Suptd.,Ship Staff","Suptd. Insp.","5s (stbd manifold) blank 2 nos bolt missing","Deck - Pipe / Fittings","Cargo / Ballast Systems","External Factors,Human Error","","","","","BOLTS FOR ALL MANIFOLD BLANKS CHECKED AND MISSING ONES WERE FIXED BACK.","2019-07-30","","Completed","2019-07-28","No","No","No","Internal"]
[null,null,null,null,8565,"86_Thu Dec 12 2019 00:26:03 GMT+0000 (Coordinated Universal Time)","2019-07-20","Defect","Owner / Marine / Tech. Suptd.,Ship Staff","Suptd. Insp.","Spanner for ISC missing at manifold","LSA / FFA","Safety / LSA / FFA","External Factors,Human Error","","","","","NEW SPANNERS PLACED IN ISC BOX","2019-08-15","","Completed","2019-08-02","No","No","No","Internal"]
[null,null,null,null,8569,"86_Thu Dec 12 2019 16:26:58 GMT+0000 (Coordinated Universal Time)","2019-07-20","Other","Owner / Marine / Tech. Suptd.,Ship Staff","Suptd. Insp.","Record of calibration of portable gas instruments to be updated (GSM form – 14.33.00.001.00) ","Documentation","Cert. & Docu.","External Factors,Human Error","","","","","RECORD OF CALIBRATION FORM UPDATED AND UPLOADED ON PAL ON MONTHLY BASIS","2019-08-15","","Completed","2019-07-30","No","No","No","Internal"]
[null,null,null,null,8570,"86_Thu Dec 12 2019 16:32:48 GMT+0000 (Coordinated Universal Time)","2019-07-20","Other","Owner / Marine / Tech. Suptd.,Ship Staff","Suptd. Insp.","Replace various instructions posted with previous company and in Chinese with our company logo and in English language ","Accommodation","General Appearance","External Factors","","","","","ALL COMPANY POSTERS HAVE BEEN POSTED AT VARIOIUS LOCATIONS AND ALL OLD POSTERS HAVE BEEN REMOVED","2019-08-08","","Completed","2019-08-06","No","No","No","Internal"]
[null,null,null,null,8575,"86_Thu Dec 12 2019 17:07:10 GMT+0000 (Coordinated Universal Time)","2019-07-20","Defect","Owner / Marine / Tech. Suptd.,Ship Staff","Suptd. Insp.","To check if all manifold drains have caps ","Deck - Pipe / Fittings","Cargo / Ballast Systems","External Factors,Human Error","","","","","ALL MANIFOLD DRAIN CAPS CHECKED. MISSING ONES WERE PUT IN PLACE.","2019-08-20","","Completed","2019-08-10","No","No","No","Internal"]
[null,null,null,null,8576,"86_Thu Dec 12 2019 17:02:11 GMT+0000 (Coordinated Universal Time)","2019-07-20","Defect","Owner / Marine / Tech. Suptd.,Ship Staff","Suptd. Insp.","No-4 foam monitor jet/spray nozzle handle missing and nozzle hard to change from jet to spray mode ","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","NEW NOZZLE REPLACED AT NO.4 FOAM MONITOR ","2019-08-08","","Completed","2019-08-04","No","No","No","Internal"]
[null,null,null,null,8577,"86_Thu Dec 12 2019 17:29:31 GMT+0000 (Coordinated Universal Time)","2019-07-20","Defect","Owner / Marine / Tech. Suptd.,Ship Staff","Suptd. Insp.","Gangway angle indicator frozen ","Deck - Machinery","ISM Related","Equipment Related","","","","","FROZEN GANGWAY ANGLE INDICATOR HAS BEEN FREED AND FOUND IN GOOD ORDER. ","2019-08-30","","Completed","2019-08-23","No","No","No","Internal"]
[null,null,null,null,8578,"86_Thu Dec 12 2019 17:34:01 GMT+0000 (Coordinated Universal Time)","2019-07-20","Defect","Owner / Marine / Tech. Suptd.,Ship Staff","Suptd. Insp.","Sprinkler valve for life boat  not operating ","LSA / FFA","Safety / LSA / FFA","Equipment Related,External Factors","","","","","SPRINKLER VALVE REPLACED BY NEW ONE AND CHECKED FOR OPERATION, ALL FOUND IN GOOD ORDER.","2019-08-27","","Completed","2019-08-20","No","No","No","Internal"]
[null,null,null,null,8579,"86_Thu Dec 12 2019 17:37:21 GMT+0000 (Coordinated Universal Time)","2019-07-20","Defect","Owner / Marine / Tech. Suptd.,Ship Staff","Suptd. Insp.","Error (20bar) in high pressure gauge for pressure regulator ","LSA / FFA","Safety / LSA / FFA","Equipment Related,External Factors","","","","","PRESSURE GUAGE READING RECTIFIED AND FOUND IN GOOD ORDER","2019-08-27","","Completed","2019-08-22","No","No","No","Internal"]
[null,null,null,null,8572,"86_Thu Dec 12 2019 16:50:29 GMT+0000 (Coordinated Universal Time)","2019-07-21","Other","Owner / Marine / Tech. Suptd.,Ship Staff","Suptd. Insp.","Upper deck toilet not operational ","Accommodation","MLC Related","Equipment Related","","","","","UPPER DECK VACCUM SYSTEM REPAIRED AND CHECKED. FOUND OPERATIONAL.","2019-08-20","","Completed","2019-08-10","No","No","No","Internal"]
[null,null,null,null,3074,"86_23/10/2019 7:16:18 AM","2019-07-23","Defect","Ship Staff","Ship Staff Insp.","MAIN ENGINE EXHAUST GAS LEAKING FROM THE EXHAUST MANIFOLD","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","",""," EXHAUST MANIFOLD DOOR OPENED , INSPECTED AND RENEWED THE GASKET","2019-08-25","","Completed","2019-08-21","No","No","No","Internal"]
[null,null,null,null,8545,"86_Thu Dec 12 2019 12:53:59 GMT+0000 (Coordinated Universal Time)","2019-07-23","Defect","Ship Staff","Ship Staff Insp.","1.\tGreasing of fwd and aft gripe wires for lifeboat at ends","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","Greasing Carried out ","2019-08-30","","Completed","2019-07-30","No","No","No","Internal"]
[null,null,null,null,8550,"86_Tue Nov 12 2019 21:39:31 GMT+0000 (Coordinated Universal Time)","2019-07-23","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Various stencils on deck have become faded and needs to be redone","Miscellaneous","General Appearance","External Factors","","","","","STENCILLING CARRIED OUT AT VARIOUS LOCATIONS ON DECK AND FADED ONES WERE RENEWED.","2019-09-10","","Completed","2019-08-30","No","No","No","Internal"]
[null,null,null,null,3050,"86_23/10/2019 3:25:44 PM","2019-07-24","Condn of Class / Memo","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","Vessel was issued following 'Outstanding Recommendation' in class","Hull & Tanks","Cert. & Docu.","External Factors","2.7","High","","","Outstanding Recommendation from Class has been closed in Drydock. ","2019-12-30","","Completed","2020-01-15","Yes","No","No","External"]
[null,null,null,null,3051,"86_23/10/2019 3:30:16 PM","2019-07-24","Defect","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","Topside hull on stb'd side was noted to be moderately rusted with","Hull & Tanks","General Appearance","External Factors","11.1","High","","","COMPLETE PAINTIN OF HULL CARRIED OUT IN DRYDOCK ","2019-11-30","","Completed","2020-01-15","Yes","No","No","External"]
[null,null,null,null,3084,"86_23/10/2019 10:02:07 AM","2019-07-26","Defect","Ship Staff","Ship Staff Insp.","FWD AIR HORN IS NOT WORKING","Miscellaneous","Emgcy. Systems","Equipment Related","","","","","REMOVED FROM PLACE DISMANTLED FOUND BEARINGS SEIZED SAME AS RENEWED AND PUT BACK , MADE OPERATIONAL","2019-08-30","","Completed","2019-08-20","No","No","No","Internal"]
[null,null,null,null,3099,"86_2019-09-10 10:02:13.000","2019-07-28","Defect","Ship Staff","Ship Staff Insp.","GARBAGE BINS ARE NOT PROVIDED IN ALL CABINS","Accommodation","General Appearance","Inappropriate Procedure","6.2","High","","","NEW GARBAGE BINS SUPPLIED AT YEOSU. ","2019-07-28","","Completed","2019-11-20","No","No","No","Internal"]
[null,null,null,null,8496,"86_Wed Oct 09 2019 10:02:13 GMT+0000 (Coordinated Universal Time)","2019-07-28","Defect","Ship Staff","Ship Staff Insp.","GARBAGE BINS ARE NOT PROVIDED IN ALL CABINS","Accommodation","General Appearance","Inappropriate Procedure","6.2","High","","","New Garbage bins received on board and same provided in all cabins.","2019-12-28","","Completed","2019-11-23","No","No","No","Internal"]
[null,null,null,null,3085,"86_23/10/2019 10:31:05 PM","2019-07-29","Defect","Ship Staff","Ship Staff Insp.","TESTING RECORD LABELS ON FEW SCBA BOTTLES IN THE CABINS MISSING. MASTER EXPALINED THAT DUE TO LACK OF LABELS ALL SCBA BOTTLES ARE NOT MARKED BUT CERTIFICATES ARE AVAILABLE","LSA / FFA","Safety / LSA / FFA","Human Error","","","","","ALL BOTTLES CHECKED AND LABELS PASTED ACCORDINGLY","2019-07-29","","Completed","2019-07-29","No","No","No","Internal"]
[null,null,null,null,3080,"86_23/10/2019 9:34:16 AM","2019-08-13","Defect","Ship Staff","Ship Staff Insp.","MAIN ENGINE #2 UNIT PUNCTURE VALVE LEAKING","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","REPLACED THE PUNCTURE VALVE WITH OVERHAULED ONE","2019-08-30","","Completed","2019-08-22","No","No","No","Internal"]
[null,null,null,null,8537,"86_24/10/2019 7:02:47 AM","2019-08-13","Defect","Ship Staff","Ship Staff Insp.","Provision crane fuse getting blown up as we start to boom up","Deck - Machinery,Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","Checked all the ckt diagram all found in good order, open juction box found rusti and water, same cleaned, changed gaskets.","2019-08-18","","Completed","2019-08-14","No","No","No","Internal"]
[null,null,null,null,3079,"86_23/10/2019 9:23:44 AM","2019-08-14","Defect","Ship Staff","Ship Staff Insp."," OBSERVED SOME ABNORMAL NOISE FROM THE ACCOMDATION A/C FAN ","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","STOPPED THE FAN INSPECTED FOUND NOISE COMING OUT OF THE BEARINGS, SO RENEWED THE BEARINGS AND TRIED OUT FOUND SMOOTH OPERATION","2019-09-30","","Completed","2019-08-26","No","No","No","Internal"]
[null,null,null,null,8568,"86_Thu Dec 12 2019 00:39:31 GMT+0000 (Coordinated Universal Time)","2019-08-18","Other","Owner / Marine / Tech. Suptd.,Ship Staff","Suptd. Insp.","Summary of tank inspection record to be updated (GSM form-DNV tank inspection form )","Documentation","Cert. & Docu.","Human Error,Inappropriate Procedure","","","","","ALL INSPECTION FOR TANKS MADE AS GSM FORM (DNV INSPECTION FORM)","2019-08-23","","Completed","2019-08-25","No","No","No","Internal"]
[null,null,null,null,3082,"86_23/10/2019 9:47:16 AM","2019-08-20","Defect","Ship Staff","Ship Staff Insp.","INCINERATOR MILL PUMP LEAKING FROM THE MECHANICAL SEAL","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","PUMP TO DISMANTLE AND REPLACE THE MECHANICAL SEAL","2019-08-30","","Completed","2019-08-28","No","No","No","Internal"]
[null,null,null,null,3105,"86_2019-10-10 10:03:28.000","2019-08-20","Defect","Ship Staff","Ship Staff Insp.","SIGNAL LIGHT COLUMN IN ER BOTTOM PLATFORM IS NOT WORKING","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","SPARES RECEIVED AND FIXED IN PLACE","2019-11-30","VIRG190028","Completed","2019-09-08","No","No","No","Internal"]
[null,null,null,null,8501,"86_Thu Oct 10 2019 10:03:28 GMT+0000 (Coordinated Universal Time)","2019-08-20","Defect","Ship Staff","Ship Staff Insp.","SIGNAL LIGHT COLUMN IN ER BOTTOM PLATFORM IS NOT WORKING","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","spare received and renewed.","2019-11-30","VIRG190028","Completed","2019-09-08","No","No","No","Internal"]
[null,null,null,null,8536,"86_24/10/2019 6:32:23 AM","2019-08-28","Defect","Ship Staff","Ship Staff Insp.","Cargo tank high level alarm not working","Cargo Mach.,Hull & Tanks","Cargo / Ballast Systems","Equipment Related","","","","","checked ckt found one fuse and relay defective same renwed","2019-08-29","","Completed","2019-08-29","No","No","No","Internal"]
[null,null,null,null,8510,"86_24/10/2019 6:38:17 AM","2019-08-29","Other","Ship Staff","Ship Staff Insp.","MSB alarm buzzer not working","Elect. Mach. & Equip.","Communication","Equipment Related","","","","","renewed with new one","2019-09-29","VIRG190050","Completed","2019-09-06","No","No","No","Internal"]
[null,null,null,null,3106,"86_2019-10-10 10:08:17.999","2019-08-31","Breakdown","Ship Staff","Ship Staff Insp.","AHU FAN SHAFT COUPLING IS CRACKED","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","renwed","2019-11-30","VIRG195099","Completed","2019-11-30","No","No","No","Internal"]
[null,null,null,null,8502,"86_Thu Oct 10 2019 10:08:17 GMT+0000 (Coordinated Universal Time)","2019-08-31","Breakdown","Ship Staff","Ship Staff Insp.","AHU FAN SHAFT COUPLING IS CRACKED","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","rectified in drydock.","2019-11-30","VIRG195099","Completed","2020-01-07","No","No","No","Internal"]
[null,null,null,null,8513,"86_24/10/2019 7:27:35 AM","2019-09-01","Defect","Ship Staff","Ship Staff Insp.","fire control station exh fan not working","Elect. Mach. & Equip.,Miscellaneous","Safety / LSA / FFA","Equipment Related","","","","","rectified.","2019-11-07","","Completed","2019-09-03","No","No","No","Internal"]
[null,null,null,null,8518,"86_16/12/2019 6:27:03 PM","2019-09-01","Defect","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","SHIP DESIGN MBL WAS 67 T LINE DESIGN  BREAK FORCE OF SIX MOORING LINES PROVIDED ON DRUMS AND IN USE WAS 60.3 T LDBF OF THESE MOORING LINES WERE NOT OF 100-105 % OF THE SHIPDESIGN MBL","Deck - Mooring Machinery","Mooring","Equipment Related","9.5","High","","","NEW MOORING ROPES SUPPLIED IN DRYDOCK WITH 67 TONS BREAK LOAD. ","2019-11-30","","Completed","2020-01-08","No","No","No","External"]
[null,null,null,null,8539,"86_24/10/2019 7:30:07 AM","2019-09-01","Defect","Ship Staff","Ship Staff Insp.","DG#2 fuel oil leak off alarm not working","E/R - Aux. Engine,Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","checked found float switch is not working same renewed","2019-09-05","","Completed","2019-09-01","No","No","No","Internal"]
[null,null,null,null,8583,"86_16/12/2019 7:05:16 PM","2019-09-01","Critical Equipment,Defect","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","PRESSURE SENSOR INDICATOR OF SLOP S IN CCR FOUND OUT OF ORDER","Cargo Mach.,Critical Equip.","Cargo / Ballast Systems","Equipment Related","8.13","Low","","","REQUISITION RAISED , NEW PRESSURE SENSOR RECEIVED  AND RENEWED ","2019-12-30","","Completed","2019-10-30","No","No","No","External"]
[null,null,null,null,8588,"86_16/12/2019 6:48:34 PM","2019-09-01","Condn of Class / Memo","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","CLASS STATUS REPORT- ONE CLASS OUTSTANDING RECOMMENDATION       1. FOREPEAK TANK , 2. NO1 WBT (S) , 3. NO2 WBT (S) ","Hull & Tanks","Structural Condn. / WT integrity ","External Factors","2.7","High","","","REPAIRS TO BE CARRIED OUT AT DRYDOCK","2020-01-27","","Completed","2019-12-09","Yes","No","No","External"]
[null,null,null,null,8589,"86_16/12/2019 7:16:00 PM","2019-09-01","Defect","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","PORT SIDE HULL OBSERVED HAVING COATING BREADKDOWN DUE TO ABBRASION ND FORMATION OF RUST EVIDENT","Hull & Tanks","Structural Condn. / WT integrity ","External Factors","11.1","High","","","HULL PAINTING AND REPAIR WORK TO BE CARRIED OUT IN DRYDOCK","2020-01-27","","Completed","2019-12-09","Yes","No","No","External"]
[null,null,null,null,8590,"86_16/12/2019 7:27:08 PM","2019-09-01","Defect","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","TOPSIDE HULL ON STBD SIDE WAS NOTED TO BE RUSTED ","Hull & Tanks","Structural Condn. / WT integrity ","External Factors","11.4","Very High","","","HULL PAINTING TO BE CARRIED OUT AT DRYDOCK","2020-01-27","","Completed","2019-12-10","Yes","No","No","External"]
[null,null,null,null,8591,"86_16/12/2019 7:20:42 PM","2019-09-01","Condn of Class / Memo,Defect","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","outstanding recommendation in class status report","Hull & Tanks","Structural Condn. / WT integrity ","External Factors","2.7","High","","","OUTSTANDING RECOMMENDATION IN CLASS STATUS REPORT","2020-01-27","","Completed","2019-12-10","Yes","No","No","External"]
[null,null,null,null,8593,"86_16/12/2019 7:24:25 PM","2019-09-01","Defect","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","REFERENCE THERMOMETER AND STANDARD PRESSURE GAUGE NOT AVAILABLE 0NBOARD","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.13","Low","","","REQUISTION RAISED , AWAITING SUPPLY","2019-11-27","","Completed","2019-10-05","No","No","No","External"]
[null,null,null,null,3052,"86_23/10/2019 3:35:20 PM","2019-09-01","Non Conformity","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","mooring lines were not of 100-105% of the Ship Design MBL","Miscellaneous,Deck - Mooring Machinery","Mooring","Inappropriate Procedure","9.5","High","","","NEW MOORING ROPES OF MBL 67 TONS SUPPLIED IN DRYDOCK AT ZHOUSHAN. ","2019-11-30","","Completed","2020-01-10","No","No","No","External"]
[null,null,null,null,8514,"86_29/10/2019 10:06:42 AM","2019-09-08","Defect","Ship Staff","Ship Staff Insp.","Galley AC is not working","Accommodation","MLC Related","Equipment Related","","","","","renewed and rectified.","2019-11-22","","Completed","2019-09-09","No","No","No","Internal"]
[null,null,null,null,3081,"86_23/10/2019 9:41:22 AM","2019-09-10","Defect","Ship Staff","Ship Staff Insp.","EXHAUST GAS BOILER MANOMETER WATER LEVEL NOT SHOWING CORRECTLY , SUSPECTING THE LINES WERE CHOKED","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","ISOLATE AND CHECKED AND FOUND BLOCKAGES, SAME CLEARED AND MADE OPERATIONAL","2019-09-30","","Completed","2019-09-22","No","No","No","Internal"]
[null,null,null,null,8540,"86_24/10/2019 7:33:49 AM","2019-09-10","Critical Equipment,Defect","Ship Staff","Ship Staff Insp.","STBD side life boat battery is not charging","LSA / FFA","Emgcy. Systems","Equipment Related","","","","","checked found wire got cut same repaired","2019-09-14","","Completed","2019-09-10","No","No","No","Internal"]
[null,null,null,null,8538,"86_24/10/2019 7:08:28 AM","2019-09-12","Defect","Ship Staff","Ship Staff Insp.","220 V feeder panel showing zero insulation because of faulty receptacle","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related,Human Error","","","","","renewed receptacle and given proper training to crew.","2019-09-18","","Completed","2019-09-13","No","No","No","Internal"]
[null,null,null,null,3078,"86_23/10/2019 9:18:22 AM","2019-09-13","Defect","Ship Staff","Ship Staff Insp.","MAIN ENGINE LUB OIL AUTO BACK WASH FILTER LEAKING FROM MOTOR COUPLING SIDE AND ALSO LEAKING FROM THE AIR CHAMBER CONNECTING UNIT TO ACTUATOR","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","PLANING TO ISOLATE DRAIN AND REMOVE THE MOTOR AND AIR CHAMBERS INSPECT AND CHANGE O-RINGS","2019-09-30","","Completed","2019-09-19","No","No","No","Internal"]
[null,null,null,null,8511,"86_24/10/2019 6:47:57 AM","2019-09-19","Defect","Ship Staff","Ship Staff Insp.","one of the Hospital call alarm push button not working","Elect. Mach. & Equip.,LSA / FFA","Communication","Equipment Related","","","","","renewed and rectified.","2019-10-07","","Completed","2019-10-05","No","No","No","Internal"]
[null,null,null,null,8512,"86_24/10/2019 6:56:07 AM","2019-09-25","Other","Ship Staff","Ship Staff Insp.","One flood light is not working at Aft deck","Elect. Mach. & Equip.","General Appearance","Equipment Related","","","","","renewed and rectified.","2019-11-08","VIRG190050","Completed","2019-10-01","No","No","No","Internal"]
[null,null,null,null,8584,"86_24/10/2019 8:24:37 AM","2019-10-02","Defect","Ship Staff","Ship Staff Insp.","Atmospheric condensor sea water inlet valve not holding","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Valve removed and replaced with the new one","2019-12-20","","Completed","2019-12-08","No","No","No","Internal"]
[null,null,null,null,3118,"86_23/10/2019 8:56:18 AM","2019-10-04","Defect","Ship Staff","Ship Staff Insp.","AUX BOILER FWD GUAGE GLASS STEAM AND WATER INLET VALVES WERE NOT HOLDING ","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","REPLACED WITH NEW ONE, RECTIFIED.","2019-11-24","","Completed","2019-11-15","No","No","No","Internal"]
[null,null,null,null,8515,"86_29/10/2019 12:22:24 PM","2019-10-04","Non Conformity","Ship Staff","Ship Staff Insp.","NAVIGATION LIGHT PANEL IN BRIDGE NOT WORKING","Navigation - Others","Navigation","External Factors","","","","","NAVIGATIONAL LIGHT PANEL SPARES RECEIVED AND NOW OPERATIONAL. ","2019-11-15","","Completed","2019-12-20","No","No","No","Internal"]
[null,null,null,null,3048,"86_23/10/2019 10:44:49 AM","2019-10-05","Defect","Ship Staff","Ship Staff Insp.","NITROGEN GENERATOR 0XYZEN SENSOR SHOWS CALIBRATION ERROR","Cargo Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","RECTIFIED BY SHORE STAFF","2019-11-25","","Completed","2020-01-05","No","No","No","Internal"]
[null,null,null,null,8516,"86_29/10/2019 12:26:30 PM","2019-10-09","Non Conformity","Ship Staff","Ship Staff Insp.","ISOLATION VALVE FOR FIRE AND FOAM LINE NOT HOLDING , ONE EACH\t\t","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","spare received and renewed.","2019-11-15","","Completed","2019-12-14","No","No","No","Internal"]
[null,null,null,null,3119,"86_23/10/2019 9:02:39 AM","2019-10-10","Defect","Ship Staff","Ship Staff Insp.","DECK SEAL PUMP SEA WATER INLET VALVE BEFORE THE FILTER WAS NOT HOLDING","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","INLET VALVE REPLACED WITH NEW ONE AND FOUND HOLDING.","2019-12-30","","Completed","2019-12-13","No","No","No","Internal"]
[null,null,null,null,3049,"86_23/10/2019 10:48:03 AM","2019-10-15","Defect","Ship Staff","Ship Staff Insp.","DECK SEAL SEA WATER PIPE LINE LEAKING , AND PIPE CONDITION IS NOT SO GOOD","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Deck seal inlet line fabrication carried out and found operational","2019-12-30","","Completed","2019-12-11","No","No","No","Internal"]
[null,null,null,null,3117,"86_23/10/2019 7:40:24 AM","2019-10-21","Defect","Ship Staff","Ship Staff Insp.","HEATING COIL OF THE BILGE HOLDING TANK FOUND WASTED COMPLETELY","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","RENEWED AND RECTIFIED","2019-12-30","","Completed","2019-11-12","No","No","No","Internal"]
[null,null,null,null,8592,"86_Mon Nov 04 2019 07:42:00 GMT+0000 (Coordinated Universal Time)","2019-11-03","Other","Ship Staff","Ship Staff Insp.","A-deck and Bridge water fountain not cooling","Miscellaneous","MLC Related","Equipment Related","","","","","Checked on A-deck found refrigerent R134a need to be charged which is not on board, Bridge water fountain's compressor renewed ","2019-11-19","","Completed","2019-12-10","No","No","No","Internal"]
[null,null,null,null,8585,"86_19/12/2019 11:09:26 AM","2019-11-08","Breakdown","Ship Staff","Ship Staff Insp.","REFRACTORY OF INCINERATOR FOUND IN DAMAGED CONDITION","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","REFRACTORY RENEWED AND SERIVICING CARRIED OUT IN DRY DOCK ","2019-12-30","","Completed","2019-12-19","Yes","No","No","Internal"]
[null,null,null,null,8587,"86_20/12/2019 10:08:08 AM","2019-11-16","Other","Ship Staff","Ship Staff Insp.","Sea water inlet valve to atmospheric condenser is not hoilding","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Renew valve with spare one","2019-12-23","","Completed","2019-12-13","No","No","No","Internal"]
[null,null,null,null,10072,"86_20/1/2020 8:41:41 PM","2019-12-02","Observation","Owner / Marine / Tech. Suptd.","Nav Audit / Verification","THE ARRIVAL DRAFT AND TRIM INFORMATION WAS MISSING IN THE PILOT CARD ","Documentation","Navigation","Human Error","","","","","PILOT CARD INFORMATION WAS COMPLETED AND MASTER TO CROSS CHECKS THE PILOT CARD INFORMATION BEFORE SIGNING. ","2019-12-09","","Completed","2019-12-05","No","No","No","Internal"]
[null,null,null,null,10073,"86_20/1/2020 9:00:13 PM","2019-12-02","Observation","Owner / Marine / Tech. Suptd.","Nav Audit / Verification","THE TELEGRAPH PRINTER TIMING WAS OFF BY ABOUT 4 MINS FROM SHIPS CLOCKS ","Navigation - Others","Navigation","Human Error","","","","","THE TIMING WAS SYNCHRONIZED WITH SHIPS CLOCKS. DUTY TO CHECK DURING CONTROL TESTS. ","2019-12-09","","Completed","2020-01-13","No","No","No","Internal"]
[null,null,null,null,10074,"86_20/1/2020 9:03:52 PM","2019-12-02","Observation","Owner / Marine / Tech. Suptd.","Nav Audit / Verification","OOW WAS NOT AWARE LOCATION OF STORAGE OF DAYLIGHT SIGNALS","Navigation - Others","Navigation","Knowledge Based","","","","","OOW WAS FAMLIARIZED WITH LOCATION OF STORAGE OF DAYLIGHT SIGNALS. ","2019-12-09","","Completed","2020-01-13","No","No","No","Internal"]
[null,null,null,null,8586,"86_20/12/2019 10:04:56 AM","2019-12-09","Other","Ship Staff","Ship Staff Insp.","Steam inlet pipe line to cascade tank is in corroded & damaged condition","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","new pipeline fabricated & fitted","2019-12-12","","Completed","2019-12-10","No","No","No","Internal"]
[null,null,null,null,null,"86_03-04-2020 17:21:09","2020-01-20","Observation","Ship Staff","Ship Staff Insp.","Dg#3fuel oil steam tracing line leaking","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related",null,null,"Not Applicable","Not Applicable","isolate the steam, remove the copper pipe and replace wit the new one","2020-01-22",null,"Completed","2020-01-21","No",null,null,"Internal"]
[null,null,null,null,null,"86_05-04-2020 13:12:59","2020-01-20","Defect","Ship Staff","Ship Staff Insp.","DECK SEAL SEA WATER PUMP DEVOLOPING PRESSURE BUT DECK SEAL IS NOT MAINTAINING ENOUGH WATER TO START IGG","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related",null,null,"Not Applicable","Not Applicable","INSPECTED AND FOUND THE SECTION OF THE PIPE IN THE ENGINE SEEMS TO BE BLOCKED SAME AS REMOVED AND CLEARED AND FITTED BACK TRIED OUT FOUND GOOD","2020-01-25",null,"Completed","2020-01-22","No",null,null,"Internal"]
[null,null,null,null,null,"86_31-03-2020 07:22:34","2020-01-27","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","The renewed Bollards to be primered and painted and stencilled for SWL.","Deck - Mooring Machinery","Mooring","Equipment Related",null,null,"Not Applicable","Not Applicable","The renewed Bollards primered and painted. SWL stenciled carried out. ","2020-02-08",null,"Completed","2020-02-04","No",null,null,"Internal"]
[null,null,null,null,null,"86_31-03-2020 07:28:06","2020-01-27","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","All hot work carried out on maindeck to be primered and painted.","Deck - Pipe / Fittings","General Appearance","Equipment Related",null,null,"Not Applicable","Not Applicable","All hot work carried out on main deck primered and painted.","2020-02-25",null,"Completed","2020-02-10","No",null,null,"Internal"]
[null,null,null,null,null,"86_31-03-2020 07:32:11","2020-01-27","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","BWTS fitted onboard room to be painted and all primered areas to be touched up.","Deck - Machinery","General Appearance","Human Error",null,null,"Not Applicable","Not Applicable","BWTS fitted onboard room fully painted.","2020-02-28",null,"Completed","2020-02-05","No",null,null,"Internal"]
[null,null,null,null,null,"86_31-03-2020 07:35:31","2020-01-27","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","U clamps on the Steam lines to be renewed and maintenance to be carried out on the steam line","Deck - Pipe / Fittings","General Appearance","Equipment Related",null,null,"Not Applicable","Not Applicable","U clamps on the Steam lines renewed and maintenance to be carried out on the steam line.","2020-02-28",null,"Completed","2020-02-12","No",null,null,"Internal"]
[null,null,null,null,null,"86_31-03-2020 07:37:37","2020-01-27","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Midship stores to be cleaned and painted.","Miscellaneous","General Appearance","Human Error",null,null,"Not Applicable","Not Applicable","Midship stores cleaned and painted.","2020-02-20",null,"Completed","2020-02-01","No",null,null,"Internal"]
[null,null,null,null,null,"86_31-03-2020 07:40:07","2020-01-27","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Tank cleaning heater Lagging to be renewed as required.","Deck - Pipe / Fittings","Safety / LSA / FFA","Equipment Related",null,null,"Not Applicable","Not Applicable","Tank cleaning heater Lagging  renewed as required.","2020-02-28",null,"Completed","2020-02-05","No",null,null,"Internal"]
[null,null,null,null,null,"86_31-03-2020 07:43:16","2020-01-27","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","All paint damage on the main deck to be buffed and painted.","Deck - Machinery","General Appearance","Equipment Related",null,null,"Not Applicable","Not Applicable","All paint damage on the main deck  buffed and painted.","2020-03-20",null,"Completed","2020-02-20","No",null,null,"Internal"]
[null,null,null,null,null,"86_31-03-2020 07:46:03","2020-01-27","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Mooring ropes to be renewed and update the Mooring matrix.","Deck - Mooring Machinery","Mooring","Inappropriate Procedure",null,null,"Not Applicable","Not Applicable","Mooring ropes renewed and update the Mooring matrix.","2020-03-30",null,"Completed","2020-03-05","No",null,null,"Internal"]
[null,null,null,null,null,"86_31-03-2020 07:49:21","2020-01-27","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","MSMP is older version.  Also update the Ship Particular page.","Deck - Mooring Machinery","Mooring","Human Error",null,null,"Not Applicable","Not Applicable","MSMP updated along with ship's particular page.","2020-02-28",null,"Completed","2020-02-01","No",null,null,"Internal"]
[null,null,null,null,null,"86_31-03-2020 07:52:07","2020-01-27","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","All Vessel certificate files index to be updated and expired certs to be removed","Documentation","Cert. & Docu.","Human Error",null,null,"Not Applicable","Not Applicable","All Vessel certificate files index updated and expired certs to be removed.","2020-02-28",null,"Completed","2020-02-01","No",null,null,"Internal"]
[null,null,null,null,null,"86_31-03-2020 08:00:29","2020-01-27","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Enclosed space entry permits please carry out training and confirm compliance as discussed","Documentation","Safety / LSA / FFA","Inappropriate Procedure",null,null,"Not Applicable","Not Applicable","Enclosed space entry permits training carry out and confirm compliance as procedure.","2020-02-28",null,"Completed","2020-02-03","No",null,null,"Internal"]
[null,null,null,null,null,"86_31-03-2020 08:03:54","2020-01-27","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Lifeboats RR tapes to be renewed and additional to be fitted.","LSA / FFA","Safety / LSA / FFA","Human Error",null,null,"Not Applicable","Not Applicable","Lifeboats RR tapes renewed and additional fitted.","2020-02-28",null,"Completed","2020-02-12","No",null,null,"Internal"]
[null,null,null,null,null,"86_31-03-2020 08:06:20","2020-01-27","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Brake rendering test date to renew as wrongly put 30 Dec 2020.","Deck - Mooring Machinery","Mooring","Human Error",null,null,"Not Applicable","Not Applicable","Brake rendering test date renewed. New stenciled of 30 Dec 2019 carried out.","2020-02-28",null,"Completed","2020-02-05","No",null,null,"Internal"]
[null,null,null,null,null,"86_31-03-2020 08:08:27","2020-01-27","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","All stencilling and markings to improve on main deck.","Cargo Mach.","General Appearance","Human Error",null,null,"Not Applicable","Not Applicable","All stencilling and markings  improved on main deck.","2020-02-28",null,"Completed","2020-02-05","No",null,null,"Internal"]
[null,null,null,null,null,"86_31-03-2020 08:22:27","2020-01-27","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","MOT ladder not in used to be marked.","Miscellaneous","General Appearance","Equipment Related",null,null,"Not Applicable","Not Applicable","MOT ladder not in used marked.","2020-02-28",null,"Completed","2020-02-02","No",null,null,"Internal"]
[null,null,null,null,null,"86_31-03-2020 08:25:58","2020-01-27","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","IMO symbols to be put in engine room for exit as discussed.","LSA / FFA","Safety / LSA / FFA","Inappropriate Procedure",null,null,"Not Applicable","Not Applicable","IMO symbols put in engine room for exit.","2020-02-28",null,"Completed","2020-02-03","No",null,null,"Internal"]
[null,null,null,null,null,"86_31-03-2020 08:40:22","2020-01-27","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","OWS filter casing to be checked for pin hole.","E/R - Pipes/ valves & fittings","MARPOL Related","Equipment Related",null,null,"Not Applicable","Not Applicable","OWS filter casing checked for pin hole and rectified.","2020-02-28",null,"Completed","2020-02-03","No",null,null,"Internal"]
[null,null,null,null,null,"86_31-03-2020 08:44:10","2020-01-27","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Lifebouy lights kindly order for intrinsically safe and renew all as present ones are not in good condition.","LSA / FFA","Safety / LSA / FFA","Equipment Related",null,null,"Not Applicable","Not Applicable","Lifebouy lights renewed where required.","2020-03-31",null,"Completed","2020-03-21","No",null,null,"Internal"]
[null,null,null,null,null,"86_31-03-2020 08:45:57","2020-01-27","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Lifeboat sight glass to be cleaned with soap water.","LSA / FFA","Safety / LSA / FFA","Equipment Related",null,null,"Not Applicable","Not Applicable","Lifeboat sight glass cleaned with soap water.","2020-02-28",null,"Completed","2020-02-04","No",null,null,"Internal"]
[null,null,null,null,null,"86_31-03-2020 08:49:07","2020-01-27","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Enclosed space drill to be carried out simulating in actual ballast tank or other enclosed space.","Documentation","Safety / LSA / FFA","Inappropriate Procedure",null,null,"Not Applicable","Not Applicable","Enclosed space drill carried out simulating in upper stow on main deck.","2020-03-30",null,"Completed","2020-03-16","No",null,null,"Internal"]
[null,null,null,null,null,"86_31-03-2020 08:51:19","2020-01-27","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Void Spaces/ Cofferdams  to be inspected and inspection records to be updated","Documentation","Cert. & Docu.","Human Error",null,null,"Not Applicable","Not Applicable","Void Spaces/ Cofferdams inspected and inspection records to be updated in tank inspection file.","2020-02-28",null,"Completed","2020-02-02","No",null,null,"Internal"]
[null,null,null,null,null,"86_31-03-2020 08:53:50","2020-01-27","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Entry for LEL checked to be updated for all spaces including the void and cofferdams in deck log book","Miscellaneous","Cargo / Ballast Systems","Inappropriate Procedure",null,null,"Not Applicable","Not Applicable","Entry for LEL checked and updated for all spaces including the void and cofferdams in deck log book","2020-02-01",null,"Completed","2020-01-28","No",null,null,"Internal"]
[null,null,null,null,null,"86_31-03-2020 08:56:31","2020-01-27","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Gangway boards and notices to be renewed as per VIQ Guidelines","Miscellaneous","General Appearance","Inappropriate Procedure",null,null,"Not Applicable","Not Applicable","Gangway boards and notices renewed as per VIQ Guidelines","2020-02-28",null,"Completed","2020-02-18","No",null,null,"Internal"]
[null,null,null,null,null,"86_31-03-2020 08:59:18","2020-01-27","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Paint Store to be cleaned and arranged all paints shall be below the sprinkler system","Miscellaneous","Safety / LSA / FFA","Human Error",null,null,"Not Applicable","Not Applicable","Paint Store cleaned, painted and arranged all paints stowed below the sprinkler system","2020-02-28",null,"Completed","2020-02-05","No",null,null,"Internal"]
[null,null,null,null,null,"86_31-03-2020 09:01:24","2020-01-27","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Accommodation spaces to be stripped and polished","Accommodation","General Appearance","Human Error",null,null,"Not Applicable","Not Applicable","Accommodation spaces stripped and polished.","2020-02-28",null,"Completed","2020-02-20","No",null,null,"Internal"]
[null,null,null,null,null,"86_31-03-2020 09:03:52","2020-01-27","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Gas meters calibration records must be as per attached format","Documentation","Cert. & Docu.","Human Error",null,null,"Not Applicable","Not Applicable","Gas meters calibration records as per company format","2020-02-20",null,"Completed","2020-02-02","No",null,null,"Internal"]
[null,null,null,null,null,"86_31-03-2020 09:11:55","2020-01-27","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Kindly do the IFC reporting while vessel is trading in the piracy area Malacca /Singapore","Navigation - Others","ISPS Related","Inappropriate Procedure",null,null,"Not Applicable","Not Applicable","IFC reporting while vessel is transiting in piracy area malaca and singapore strait carried out. ","2020-03-01",null,"Completed","2020-02-08","No",null,null,"Internal"]
[null,null,null,null,null,"86_31-03-2020 09:15:33","2020-01-27","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Please check for Hardening equipment onboard as the vessel might call Africa and raise REQ","Miscellaneous","ISPS Related","Behaviour Based",null,null,"Not Applicable","Not Applicable","Hardening equipments onboard checked, for required items REQ raised. ","2020-03-30",null,"Completed","2020-03-10","No",null,null,"Internal"]
[null,null,null,null,null,"86_03-04-2020 11:32:28","2020-02-03","Defect","Ship Staff","Ship Staff Insp.","Aux boiler port side forward side guage glass broken causing steam leakage.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related",null,null,"Not Applicable","Not Applicable","Isolated the Guage glass steam and water side. dismentled and replaced with new guage glass. tested & found operational.","2020-02-06",null,"Completed","2020-02-06","No",null,null,"Internal"]
[null,null,null,null,null,"86_05-04-2020 13:19:44","2020-02-07","Defect","Ship Staff","Ship Staff Insp.","EHAUST GAS BOILER SOOT BLOWING STEAM LINE GOT HOLE ,STEAM LEAKING BADLY","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related",null,null,"Not Applicable","Not Applicable","SO ISOLATED THE STEAM AND EMOVED THE SECTION OF THE PIPE FABRICATED THE NEW ONE AND FITTED BACK , RECTIFIED LEAKAGE","2020-02-10",null,"Completed","2020-02-08","No",null,null,"Internal"]
[null,null,null,null,null,"86_05-04-2020 13:24:17","2020-02-10","Defect","Ship Staff","Ship Staff Insp.","HFO PURIFIER #1 STEAM INLET VALVE NOT HOLDING AND FOUND THE HANDLE OF THE VALVE BROKEN, ","E/R - Purifier","Eng. / Strg. Comp.","Equipment Related",null,null,"Not Applicable","Not Applicable","STARTED THE #2 PURIFIER AND STOPPED 31 PURIFIER REMOVED THE VALVE AND REPLACED WITH THE NEW ONE","2020-02-16",null,"Completed","2020-02-12","No",null,null,"Internal"]
[null,null,null,null,null,"86_05-04-2020 13:28:08","2020-02-12","Defect","Ship Staff","Ship Staff Insp.","MAIN ENGINE FUEL OIL AUTO BACK FLUSH DRAIN CHAMBER MALFUNCTIONING AND THE OVERFLOW TANK LEVEL RAISING","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related",null,null,"Not Applicable","Not Applicable","BYPASSED THE AUTO BACK FLUSH FILTER , REMOVED THE DRAIN CHAMBER PISTON FOUND O-RINGS DAMAGED SAME AS REPLACED WITH THE NEW ONES AND TRIED OUT FOUND NO LEAKAGE","2020-02-19",null,"Completed","2020-02-14","No",null,null,"Internal"]
[null,null,null,null,null,"86_05-04-2020 16:17:47","2020-02-13","Defect","Ship Staff","Ship Staff Insp.","EERGENCY FIRE PUP DISCHARGE PRESSURE GUAGE FOUND FAULTY","E/R - Aux. Mach.","Emgcy. Systems","Equipment Related",null,null,"Not Applicable","Not Applicable","REMOVED THE DEFECTIVE ONE AND REPLACED WITH THE NEW ONE","2020-03-17",null,"Completed","2020-03-15","No",null,null,"Internal"]
[null,null,null,null,null,"86_05-04-2020 15:44:07","2020-02-18","Defect","Ship Staff","Ship Staff Insp.","MAIN  COOL SEA WATER PUMP #1 AND #2 LEAKING FROM THE ANODE COVERS ","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related",null,null,"Not Applicable","Not Applicable","ISOLATED THE PUMPS ONE BY ONE AND REMOVED THE ANODE COVERS FOUND WASTAGE 70% SO RENEWED THE ANODES AND COVER GASKETS AND FITTED BACK RECTIFIED LEAKAGE","2020-02-24",null,"Completed","2020-02-20","No",null,null,"Internal"]
[null,null,null,null,null,"86_05-04-2020 15:48:27","2020-02-21","Defect","Ship Staff","Ship Staff Insp.","MDO BUNKER LINE GOT A PIN HOLE OBSERVED OIL DRIBBLING FROM IT","Deck - Pipe / Fittings","MARPOL Related","Equipment Related",null,null,"Not Applicable","Not Applicable","SYSTEM ISOLATED AND REMOVED THE SECTION OF THE PIPE AND BLANKED THE FLANGES, FABRICATED A NEW SECTION OF PIPE AND FITTED BACK IN PLACE AND RECTIFIED THE LEAKAGE","2020-02-26",null,"Completed","2020-02-22","No",null,null,"Internal"]
[null,null,null,null,null,"86_05-04-2020 15:57:05","2020-02-22","Defect","Ship Staff","Ship Staff Insp.","MAIN COOL SEA WATER PUMP TRIPPPED FOUND MOTOR IS NOT STSRTING","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related",null,null,"Not Applicable","Not Applicable","INSPECTED AND FOUND MOTOR WINDINGS GOT BURNT , RENEWED THE SEA WATER PPUMP MOTOR AND TRIED OUT  FOUND GOOD","2020-02-29",null,"Completed","2020-02-23","No",null,null,"Internal"]
[null,null,null,null,null,"86_05-04-2020 15:52:06","2020-02-23","Defect","Ship Staff","Ship Staff Insp.","BIGE PUMP RUNNING BUT NOT DISCHARGING WATER TO BILGE HOLDING TANK","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related",null,null,"Not Applicable","Not Applicable","SUSPECTED RELEIF VALVE NIT FUNCTIONING WATER RECIRCULATING, SO REMOVED THE RELEIF VALVE DISMANTLED FOUND SPRING BROKEN SAME RENEWED AND FITTED BACK TRIED OUT FOUND GOOD","2020-02-29",null,"Completed","2020-02-24","No",null,null,"Internal"]
[null,null,null,null,null,"86_05-04-2020 16:01:56","2020-02-24","Defect","Ship Staff","Ship Staff Insp.","MAIN ENGINE FUEL PUMP HIGH PRESSURE PIPE  GOING TO FUEL INJECTOR LEAKING","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related",null,null,"Not Applicable","Not Applicable","ISOLATED THE #6 UNIT FUEL PUMP REMOVED THE PIPE FOUND O-RINGS BROKEN REPLACED THEM WITH NEW O-RINGS AND TIGHTENED BACK AND RECTIFIED LEAKAGE","2020-02-29",null,"Completed","2020-02-26","No",null,null,"Internal"]
[null,null,null,null,null,"86_05-04-2020 16:05:52","2020-02-26","Defect","Ship Staff","Ship Staff Insp.","MAIN ENGINE #4 UNIT NOT FIRING WHEN ENGINE LOAD CHANGES ","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related",null,null,"Not Applicable","Not Applicable","STOPED THE MAIN ENGINE AND DISMANTLED THE #4 UNIT MAIN ENGINE FUEL PUMPP FOUND CONSIDERABLE SCORING ON PLUNGER AND BARREL , INFORMED TO OFFICE AND REPLACED WITH NEW PLUNGER AND BARREL TRIED OUT FOUND EVERTHING GOOD","2020-03-10",null,"Completed","2020-03-03","No",null,null,"Internal"]
[null,null,null,null,null,"86_05-04-2020 16:09:46","2020-03-05","Defect","Ship Staff","Ship Staff Insp.","CONTROL AIR DRYER GETTING TRIPPED DUE TO HIGH PRESSURE","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related",null,null,"Not Applicable","Not Applicable","INSPECTED FOUND EVAPORATOR  FAN NOT RUNNING SO REMOVED THE FAN AND RENEWED THE NBEARING AND ASSEMBLED BACK TRIED OUT FOUND WORKING NORMAL","2020-03-08",null,"Completed","2020-03-06","No",null,null,"Internal"]
[null,null,null,null,null,"86_05-04-2020 16:25:27","2020-03-17","Defect","Ship Staff","Ship Staff Insp.","MAIN COOL SEA WATER PUMP  DISCHARGE  SIDE NON RETURN VALVE NOT HOLDING PUMP START ROTATING IN STOP CONDITION ","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related",null,null,"Not Applicable","Not Applicable","ISOLATED THE SYSTEM CLOSED THE INLET AND OUTLET VALVES REMOVED THE NONRETURN VALVE FROM PLACE FOUND FLAP BROKEN SAME AS REPLACED WITH THE NEW ONE AND TRIED OUT FOUND VALVE HOLDING PROPERLY","2020-03-25",null,"Completed","2020-03-20","No",null,null,"Internal"]

{"sheet":"Calc","index":2,"n_rows":28,"n_cols":12,"rows_kept":28,"cut":false,"hidden":true,"merged":[]}
["Def_type","Def_cause","Equipments","VIQrefno","Observer_code"]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,"Dim itemSele As Long"]
[null,null,null,null,null,null,null,null,null,null,null,"   dim startRow as integer"]
[null,null,null,null,null,null,null,null,null,null,null,"   startRow=1"]
[null,null,null,null,null,null,null,null,null,null,null,"        For itemSele = 0 To ListBox1.ListCount - 1"]
[null,null,null,null,null,null,null,null,null,null,null,"        If ListBox1.Selected(itemSele) = True Then"]
[null,null,null,null,null,null,null,null,null,null,null,"        Worksheets(\"WorksheetName\").Range(\"A\" & startRow).Value = ListBox1.List(itemSele)"]
[null,null,null,null,null,null,null,null,null,null,null,"        startRow = startRow + 1"]
[null,null,null,null,null,null,null,null,null,null,null,"        End If"]
[null,null,null,null,null,null,null,null,null,null,null,"        Next"]
[null,null,null,null,null,null,null,null,null,null,null,"Dim LastRowA As String"]
[null,null,null,null,null,null,null,null,null,null,null,"        Dim itemSele As Long"]
[null,null,null,null,null,null,null,null,null,null,null,"       Dim startRow as integer"]
[null,null,null,null,null,null,null,null,null,null,null,"        LastRowA = ActiveSheet.Cells(Rows.count, \"A\").End(xlUp).row"]
[null,null,null,null,null,null,null,null,null,null,null,"        startQue = 0"]
[null,null,null,null,null,null,null,null,null,null,null,"        For itemSele = 0 To ListBox1.ListCount - 1"]
[null,null,null,null,null,null,null,null,null,null,null,"        For startRow = 1 To LastRowA"]
[null,null,null,null,null,null,null,null,null,null,null,"        If Worksheets(\"WorksheetName\").Range(\"A\" & startRow).Value = ListBox1.List(itemSele) Then"]
[null,null,null,null,null,null,null,null,null,null,null,"        ListBox1.Selected(itemSele) = True"]
[null,null,null,null,null,null,null,null,null,null,null,"        Exit For"]
[null,null,null,null,null,null,null,null,null,null,null,"        End If"]
[null,null,null,null,null,null,null,null,null,null,null,"        Next j"]
[null,null,null,null,null,null,null,null,null,null,null,"        Next"]
[null,null,null,null,null,null,null,null,null,null,null,"        End If"]

{"sheet":"Areaofobs","index":3,"n_rows":17,"n_cols":2,"rows_kept":17,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Cargo / Ballast Systems",11]
["Cert. & Docu.",2]
["Communication",6]
["Crew Management",3]
["Emgcy. Systems",13]
["Eng. / Strg. Comp.",14]
["General Appearance",15]
["Ice Opns.",17]
["ISM Related",7]
["ISPS Related",10]
["MARPOL Related",9]
["MLC Related",4]
["Mooring",12]
["Navigation",5]
["Safety / LSA / FFA",8]
["Structural Condn. / WT integrity ",16]

{"sheet":"Vessel_type","index":4,"n_rows":1,"n_cols":2,"rows_kept":1,"cut":false,"hidden":true,"merged":[]}
["Vessel_type","ID"]

{"sheet":"Deficiency_type","index":5,"n_rows":8,"n_cols":3,"rows_kept":8,"cut":false,"hidden":true,"merged":[]}
["TITLE","Type of deficiency_description","ID"]
["Breakdown",null,6]
["Critical Equipment",null,4]
["Defect",null,1]
["Guarantee Claim",null,8]
["Non Conformity",null,2]
["Observation",null,3]
["Other",null,7]

{"sheet":"VIQrefno","index":6,"n_rows":363,"n_cols":3,"rows_kept":363,"cut":false,"hidden":true,"merged":[]}
["VIQ_ref_no","Risk Value of observation","ID"]
["1.1","Low",8627]
["1.10","Low",8636]
["1.11","Low",8637]
["1.12","Low",8638]
["1.13","Low",8639]
["1.14","Low",8640]
["1.15","Low",8641]
["1.16","Low",8643]
["1.17","Low",8644]
["1.18","Low",8645]
["1.19","Low",8646]
["1.2","Low",8628]
["1.20","Low",8647]
["1.21","",8648]
["1.22","Low",8650]
["1.23","Low",8651]
["1.24","Low",8652]
["1.25","Low",8653]
["1.26","Low",8654]
["1.3","Low",8629]
["1.4","Low",8630]
["1.5","Low",8631]
["1.6","Low",8632]
["1.7","Low",8633]
["1.8","Low",8634]
["1.9","Low",8635]
["1.99","High",15785]
["10.1","Medium",8821]
["10.10","High",8830]
["10.11","Medium",8831]
["10.12","Very High",8832]
["10.13","Very High",8833]
["10.14","Medium",8834]
["10.15","Low",8835]
["10.16","Very High",8836]
["10.17","Very High",8837]
["10.18","High",8838]
["10.19","Very High",8839]
["10.2","Low",8822]
["10.20","High",8840]
["10.21","Medium",8841]
["10.22","Low",8842]
["10.23","Medium",8843]
["10.24","Low",8844]
["10.25","Very High",8845]
["10.26","High",8846]
["10.27","Medium",8847]
["10.28","Low",8848]
["10.29","Medium",8849]
["10.3","Medium",8823]
["10.30","High",8850]
["10.31","Very High",8851]
["10.32","Very High",8852]
["10.33","High",8853]
["10.34","High",8854]
["10.35","Very High",8855]
["10.36","Very High",8856]
["10.37","Medium",8857]
["10.38","Medium",8858]
["10.39","High",8859]
["10.4","High",8824]
["10.40","Medium",8860]
["10.41","Medium",8861]
["10.42","Medium",8862]
["10.43","Medium",8863]
["10.44","Medium",8864]
["10.45","Very High",8865]
["10.46","High",8866]
["10.47","Medium",8867]
["10.48","High",8868]
["10.49","Medium",8869]
["10.5","Low",8825]
["10.50","High",8870]
["10.51","Low",8871]
["10.52","Medium",8872]
["10.53","Medium",8873]
["10.54","High",8874]
["10.55","Low",8875]
["10.6","Very High",8826]
["10.7","Medium",8827]
["10.8","Medium",8828]
["10.9","Medium",8829]
["10.99","High",8876]
["11.1","High",8780]
["11.10","Medium",8789]
["11.11","Very High",8790]
["11.12","Low",8791]
["11.13","Low",8792]
["11.14","Medium",8793]
["11.15","Low",8794]
["11.16","Low",8795]
["11.17","Low",8796]
["11.2","Medium",8781]
["11.3","Medium",8782]
["11.4","Very High",8783]
["11.5","Medium",8784]
["11.6","Medium",8785]
["11.7","High",8786]
["11.8","Low",8787]
["11.9","Low",8788]
["11.99","High",8797]
["12.1","High",8798]
["12.10","High",8808]
["12.11","High",8809]
["12.12","High",8810]
["12.13","High",8811]
["12.14","High",8812]
["12.15","High",8813]
["12.16","High",8814]
["12.17","High",8815]
["12.18","High",8816]
["12.19","High",8817]
["12.2","High",8799]
["12.20","High",8818]
["12.21","High",8819]
["12.3","High",8801]
["12.4","High",8802]
["12.5","High",8803]
["12.6","High",8804]
["12.7","High",8805]
["12.8","High",8806]
["12.9","High",8807]
["12.99","High",8820]
["2.1","Very High",15]
["2.1.9","Very High",16]
["2.10","Medium",25]
["2.11","Medium",26]
["2.12","Medium",27]
["2.13","High",28]
["2.14","High",29]
["2.15","High",30]
["2.16","Medium",31]
["2.2","Medium",17]
["2.3","High",18]
["2.4","Medium",19]
["2.5","Low",20]
["2.6","Medium",21]
["2.7","High",22]
["2.8","Medium",23]
["2.9","Low",24]
["2.99","High",8672]
["3.1","High",8673]
["3.2","Very High",8674]
["3.3","High",8675]
["3.4","Low",8655]
["3.5","Medium",8676]
["3.6","High",8677]
["3.7","Very High",8678]
["3.8","Very High",8679]
["3.99","High",8680]
["4.1","High",8681]
["4.10","High",8690]
["4.11","Medium",8691]
["4.12","Very High",8692]
["4.13","Very High",8693]
["4.14","Very High",8694]
["4.15","Very High",8695]
["4.16","Very High",8696]
["4.17","Very High",8697]
["4.18","Very High",8698]
["4.19","Low",8699]
["4.2","Medium",8682]
["4.20","Very High",8700]
["4.21","High",8701]
["4.22","Low",8702]
["4.23","High",8703]
["4.24","High",8704]
["4.25","Low",8705]
["4.26","Low",8706]
["4.27","High",8707]
["4.3","Medium",8683]
["4.4","High",8684]
["4.5","Very High",8685]
["4.6","Medium",8686]
["4.7","High",8687]
["4.8","Medium",8688]
["4.9","Medium",8689]
["4.99","High",8708]
["5.1","Very High",8877]
["5.10","High",8886]
["5.11","Low",8887]
["5.12","Medium",8888]
["5.13","High",8889]
["5.14","Very High",8890]
["5.15","Medium",8891]
["5.16","Medium",8892]
["5.17","Very High",8893]
["5.18","High",8894]
["5.19","Medium",8895]
["5.2","Very High",8878]
["5.20","Medium",8896]
["5.21","Medium",8897]
["5.22","High",8899]
["5.23","Very High",8900]
["5.24","Very High",8901]
["5.25","Medium",8902]
["5.26","Medium",8903]
["5.27","Medium",8904]
["5.28","Very High",8905]
["5.29","High",8906]
["5.3","Low",8879]
["5.30","High",8907]
["5.31","High",8908]
["5.32","High",8909]
["5.33","High",8910]
["5.34","Low",8911]
["5.35","Medium",8912]
["5.36","Low",8913]
["5.37","Low",8914]
["5.38","High",8915]
["5.39","Very High",8916]
["5.4","High",8880]
["5.40","Very High",8917]
["5.41","Very High",8918]
["5.42","Medium",8919]
["5.43","High",8920]
["5.44","High",8921]
["5.45","Medium",8924]
["5.46","Medium",8925]
["5.47","Low",8926]
["5.48","Medium",8927]
["5.5","Low",8881]
["5.6","Low",8882]
["5.7","Medium",8883]
["5.8","Medium",8884]
["5.9","Very High",8885]
["5.99","High",8928]
["6.1","Medium",8709]
["6.10","Low",8718]
["6.11","High",8719]
["6.12","Medium",8720]
["6.13","Low",8721]
["6.14","High",8722]
["6.15","High",8723]
["6.16","Very High",8724]
["6.17","Very High",8725]
["6.18","Medium",8726]
["6.19","Low",8727]
["6.2","High",8710]
["6.20","Medium",8728]
["6.21","High",8729]
["6.22","Medium",8730]
["6.3","Low",8711]
["6.4","High",8712]
["6.5","Low",8713]
["6.6","Medium",8714]
["6.7","High",8715]
["6.8","High",8716]
["6.9","Low",8717]
["6.99","High",8731]
["7.1","High",8732]
["7.10","High",8741]
["7.11","High",8742]
["7.12","High",8743]
["7.13","Medium",8744]
["7.14","Medium",8745]
["7.15","High",8746]
["7.16","High",8747]
["7.17","High",8748]
["7.2","High",8733]
["7.3","Low",8734]
["7.4","Low",8735]
["7.5","Low",8736]
["7.6","Medium",8737]
["7.7","Low",8738]
["7.8","High",8739]
["7.9","High",8740]
["7.99","High",8749]
["8.1","Very High",8929]
["8.10","Very High",8938]
["8.11","Medium",8939]
["8.12","Medium",8940]
["8.13","Low",8941]
["8.14","Medium",8942]
["8.15","Medium",8943]
["8.16","Medium",8944]
["8.17","Medium",8945]
["8.18","Low",8946]
["8.19","Medium",8947]
["8.2","Medium",8930]
["8.20","Medium",8948]
["8.21","Medium",8949]
["8.22","Very High",8950]
["8.23","Medium",8951]
["8.24","Very High",8952]
["8.25","Medium",8953]
["8.26","Low",8954]
["8.27","Medium",8955]
["8.28","Medium",8956]
["8.29","Medium",8958]
["8.3","Medium",8931]
["8.30","Very High",8959]
["8.31","Medium",8960]
["8.32","Medium",8961]
["8.33","Very High",8962]
["8.34","High",8963]
["8.35","Medium",8964]
["8.36","Medium",8965]
["8.37","Medium",8967]
["8.38","Low",8968]
["8.39","Low",8969]
["8.4","Very High",8932]
["8.40","Very High",8970]
["8.41","Very High",8971]
["8.42","Medium",8972]
["8.43","Low",8973]
["8.44","Medium",8975]
["8.45","High",8976]
["8.46","Medium",8977]
["8.47","Medium",8978]
["8.48","Medium",8979]
["8.49","Medium",8980]
["8.5","Medium",8933]
["8.50","Very High",8981]
["8.51","Very High",8982]
["8.52","Very High",8983]
["8.53","Very High",8984]
["8.54","Medium",8985]
["8.55","Very High",15711]
["8.56","Very High",15712]
["8.57","Medium",15713]
["8.58","Medium",15714]
["8.59","Very High",15715]
["8.6","Medium",8934]
["8.60","Medium",15716]
["8.61","Low",15717]
["8.62","Medium",15718]
["8.63","Medium",15719]
["8.7","Very High",8935]
["8.8","Very High",8936]
["8.9","High",8937]
["8.99","High",15755]
["9.1","Low",8750]
["9.10","Medium",8759]
["9.11","Medium",8760]
["9.12","Medium",8761]
["9.13","Low",8762]
["9.14","Medium",8763]
["9.15","Medium",8764]
["9.16","High",8765]
["9.17","High",8766]
["9.18","Low",8767]
["9.19","Low",8768]
["9.2","Very High",8751]
["9.20","Medium",8769]
["9.21","Medium",8770]
["9.22","Low",8771]
["9.23","Low",8772]
["9.24","Medium",8773]
["9.25","Low",8774]
["9.26","Low",8775]
["9.27","Low",8776]
["9.28","Medium",8777]
["9.29","Low",8778]
["9.3","Very High",8752]
["9.4","High",8753]
["9.5","High",8754]
["9.6","Low",8755]
["9.7","Medium",8756]
["9.8","Medium",8757]
["9.9","Medium",8758]
["9.99","High",8779]

{"sheet":"Equipment_list","index":7,"n_rows":28,"n_cols":3,"rows_kept":28,"cut":false,"hidden":true,"merged":[]}
["TITLE","Equipment_list_description","ID"]
["Accommodation",null,12]
["Cargo Mach.",null,13]
["Critical Equip.",null,16]
["Deck - Machinery",null,18]
["Deck - Mooring Machinery",null,15]
["Deck - Pipe / Fittings",null,20]
["Documentation",null,21]
["E/R - Air Comp.",null,8]
["E/R - Aux. Engine",null,4]
["E/R - Aux. Mach.",null,7]
["E/R - Boiler",null,5]
["E/R - Main Engine",null,3]
["E/R - Pipes/ valves & fittings",null,9]
["E/R - Pumps",null,32]
["E/R - Purifier",null,6]
["Elect. Mach. & Equip.",null,10]
["Hull & Tanks",null,19]
["Inert Gas",null,14]
["LSA / FFA",null,17]
["Miscellaneous",null,22]
["Navigation - DGPS / EPFS / AIS",null,28]
["Navigation - ECDIS",null,25]
["Navigation - Echo Sounder / Speed Log",null,26]
["Navigation - GMDSS & Communication",null,23]
["Navigation - Others",null,11]
["Navigation - RADAR",null,24]
["Navigation - VDR / BNWAS",null,30]

{"sheet":"PSC_MOU","index":8,"n_rows":11,"n_cols":3,"rows_kept":11,"cut":false,"hidden":true,"merged":[]}
["TITLE","PSC_MOU_description","ID"]
["Asia and the Pacific",null,2]
["Caribbean",null,4]
["Europe and the North Atlantic",null,1]
["Latin America",null,3]
["The Black Sea region",null,6]
["The Indian Ocean",null,8]
["The Mediterranean",null,7]
["The Riyadh MoU",null,9]
["USCG",null,10]
["West and Central Africa",null,5]

{"sheet":"Inspection_type","index":9,"n_rows":12,"n_cols":2,"rows_kept":12,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Bunkering Audit",14]
["Cargo Audit",17]
["Engineering Audit",16]
["ISM Audit",2]
["ISPS Audit",3]
["IT Audit",10]
["MLC Audit",1]
["Mooring Audit",9]
["Nav Audit / Verification",8]
["Ship Staff Insp.",15]
["Suptd. Insp.",13]

{"sheet":"Deficiency_Cause","index":10,"n_rows":8,"n_cols":3,"rows_kept":8,"cut":false,"hidden":true,"merged":[]}
["TITLE","Deficiency_Cause_description","ID"]
["Behaviour Based",null,1]
["Equipment Related",null,4]
["External Factors",null,5]
["Human Error",null,7]
["Inappropriate Procedure",null,8]
["Industry Issue",null,6]
["Knowledge Based",null,3]

{"sheet":"Observer_code","index":11,"n_rows":3,"n_cols":3,"rows_kept":3,"cut":false,"hidden":true,"merged":[]}
["TITLE","Observer_code_description","ID"]
["Owner / Marine / Tech. Suptd.",null,3]
["Ship Staff",null,2]

{"sheet":"Status_code","index":12,"n_rows":6,"n_cols":3,"rows_kept":6,"cut":false,"hidden":true,"merged":[]}
["TITLE","Status_code_description","ID"]
["Completed",null,6]
["Deferred to D D",null,5]
["In progress",null,3]
["Not Started",null,2]
["Waiting spare",null,4]

{"sheet":"PSC_ref_no","index":13,"n_rows":19,"n_cols":2,"rows_kept":19,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Alarms",9]
["Cargo operations including equipment",7]
["Certificates & Documentation",2]
["Dangerous Goods",13]
["Emergency Systems",5]
["Fire safety",8]
["ISM",16]
["ISPS",17]
["Life saving appliances",12]
["MLC, 2006",18]
["Other",19]
["Pollution Prevention",15]
["Propulsion and auxiliary machinery",14]
["Radio communication",6]
["Safety of Navigation",11]
["Structural condition",3]
["Water/Weathertight condition",4]
["Working and Living Conditions",10]

{"sheet":"Risk_value_of_obs","index":14,"n_rows":1,"n_cols":2,"rows_kept":1,"cut":false,"hidden":true,"merged":[]}
["Risk Value of observation","ID"]

{"sheet":"Year","index":15,"n_rows":18,"n_cols":1,"rows_kept":18,"cut":false,"hidden":true,"merged":[]}
["Year"]
[2014]
[2015]
[2016]
[2017]
[2018]
[2019]
[2020]
[2021]
[2022]
[2023]
[2024]
[2025]
[2026]
[2027]
[2028]
[2029]
[2030]

{"sheet":"Month","index":16,"n_rows":13,"n_cols":1,"rows_kept":13,"cut":false,"hidden":true,"merged":[]}
["Month"]
["Jan"]
["Feb"]
["Mar"]
["Apr"]
["May"]
["Jun"]
["Jul"]
["Aug"]
["Sep"]
["Oct"]
["Nov"]
["Dec"]

{"sheet":"Date_","index":17,"n_rows":32,"n_cols":1,"rows_kept":32,"cut":false,"hidden":true,"merged":[]}
["Date"]
["01"]
["02"]
["03"]
["04"]
["05"]
["06"]
["07"]
["08"]
["09"]
[10]
[11]
[12]
[13]
[14]
[15]
[16]
[17]
[18]
[19]
[20]
[21]
[22]
[23]
[24]
[25]
[26]
[27]
[28]
[29]
[30]
[31]

{"sheet":"Sheet1","index":18,"n_rows":24,"n_cols":6,"rows_kept":24,"cut":false,"hidden":true,"merged":[]}
[]
[null,"ID","E",null,"Date Recorded",1]
[null,"UNIQUE ID","F",null,"Type of Deficiency",2]
[1,"Date Recorded","G",null,"Observer code",3]
["ignore","Vessel Type","H",null,"Type of Inspection",4]
[null,"Internal / External","I",null,"Description of Deficiency",5]
[null,"Drydock","J",null,"Equipment Categories",6]
[null,"Information Sharing","K",null,"Area of Observation",7]
[null,"Critical_item","L",null,"Deficiency Cause",8]
[null,"Deficiency Type","M",null,"VIQ Ref Number",9]
[null,"Deficiency Cause","N",null,"Risk Value of Obs",10]
[null,"Inspection Type","O",null,"PSC Ref Number",11]
[null,"Equipments","P",null,"PSC MOU ID",12]
[null,"VIQ Reference Number","Q",null,"Action Taken or Required",13]
[null,"Risk Value of the observation","R",null,"Target Date",14]
[null,"PSC Reference Number","S",null,"PO Ref No.",15]
[null,"PSC MOU","T",null,"Status Code",16]
[null,"Observer Code","U",null,"Date Completed",17]
[null,"Target Date","V",null,"Drydock",18]
[null,"Status Code","W",null,"Info Sharing",19]
[null,"Description of Deficiency","X",null,"Critical Item Flag",20]
[null,"Action taken / required","Y",null,"Audit Type",21]
[null,"PO ref no","Z"]
[null,"Date completed","AA"]

{"sheet":"Ship_information","index":19,"n_rows":2,"n_cols":3,"rows_kept":2,"cut":false,"hidden":true,"merged":[]}
["Ship_ID","Ship_Name","FILE_NAME"]
["86","VIRGO (21-01-2020)","86_1584603563285.xlsm"]

{"sheet":"External_Deficiency_type","index":20,"n_rows":5,"n_cols":3,"rows_kept":5,"cut":false,"hidden":true,"merged":[]}
["TITLE","Type of deficiency_description","ID"]
["Condn of Class / Memo",null,5]
["Defect",null,1]
["Non Conformity",null,2]
["Observation",null,3]

{"sheet":"External_Inspection_type","index":21,"n_rows":11,"n_cols":2,"rows_kept":11,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Cargo Audit",17]
["Flag State Insp.",5]
["ISM Audit",2]
["ISPS Audit",3]
["MLC Audit",1]
["Nav Audit / Verification",8]
["OM Insp. (Eg. SIRE / CDI etc.)",6]
["Others (Eg. Insurance etc.)",12]
["PSC Inspection",4]
["Terminal Insp.",11]

{"sheet":"External_Observer_code","index":22,"n_rows":7,"n_cols":3,"rows_kept":7,"cut":false,"hidden":true,"merged":[]}
["TITLE","Observer_code_description","ID"]
["Class Surveyor",null,4]
["FSC Inspector",null,5]
["Others (Eg. Insurance etc.)",null,9]
["PSC Insp.",null,6]
["SIRE / CDI Insp.",null,8]
["Terminal Insp.",null,7]

{"sheet":"Sheet Version","index":23,"n_rows":2,"n_cols":2,"rows_kept":2,"cut":false,"hidden":true,"merged":[]}
["Version","Title"]
["2.0","Version 2.0"]