{"text_format":"1","workbook":"xlsx","n_sheets":24,"sheets":["Mainsheet","Completed","Calc","Areaofobs","Vessel_type","Deficiency_type","VIQrefno","Equipment_list","PSC_MOU","Inspection_type","Deficiency_Cause","Observer_code","Status_code","PSC_ref_no","Risk_value_of_obs","Year","Month","Date_","Sheet1","Ship_information","External_Deficiency_type","External_Inspection_type","External_Observer_code","Sheet Version"],"not_rendered":{"charts":0,"images":6,"macros":1,"external_links":0,"defined_names":12,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Mainsheet","index":0,"n_rows":68,"n_cols":28,"rows_kept":68,"cut":false,"hidden":false,"merged":[[10,8,10,9],[10,12,10,13],[12,6,12,27],[8,6,8,27]]}
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,"Defect - Damage Monitoring Sheet"]
[]
[null,null,null,null,null,null,null,"Date of Report","31-Dec-2019",null,null,"Ship Name","PERFECT (26-12-2019)"]
[]
[null,null,null,null,null,null,"VERSION : 2.0"]
[]
[]
[]
[null,null,null,null,"ID","UNIQUE ID","Date Recorded","Type of Deficiency","Observer code","Type of Inspection","Description of Deficiency","Equipment Categories","Area of Observation","Deficiency Cause","VIQ Ref Number","Risk Value of Obs","PSC Ref Number","PSC MOU ID","Action Taken or Required","Target Date","PO Ref No.","Status Code","Date Completed","Drydock","Info Sharing","Critical Item","Audit Type","Superintendent Remarks"]
[null,null,null,null,9018,"99_23/12/2019 8:16:00 PM","2019-12-11","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Aft machinery hydraulic tank gauge glass cracked ","Deck - Mooring Machinery","Eng. / Strg. Comp.","Equipment Related",null,null,"Not Applicable","Not Applicable","Gauge glass to order","2020-03-11","PERF200121","Waiting spare",null,"No","No","No","Internal"]
[null,null,null,null,9022,"99_23/12/2019 10:23:28 PM","2019-11-27","Defect","Ship Staff","Ship Staff Insp.","SEVERAL CHOCKS & BOLLARDS FOUND WITH DEEP GROOVING","Deck - Pipe / Fittings","Mooring","Equipment Related",9.18,"Low","Not Applicable","Not Applicable","NEE TO BULIT UP IN DRYDOCK","2020-12-30",null,"Deferred to D D",null,"Yes","No","No","Internal"]
[null,null,null,null,9027,"99_24/12/2019 11:48:38 AM","2019-11-27","Defect","Ship Staff","Ship Staff Insp.","U CLAMPS FOR VALVE HYDRAULIC, AIR LINE & FRESH WATER LINE FOUND WASTED","Deck - Pipe / Fittings","General Appearance","Inappropriate Procedure",11.5,"Medium","Not Applicable","Not Applicable","RENEWAL IN PROGRESS","2020-06-30",null,"In progress",null,"No","No","No","Internal"]
[null,null,null,null,9036,"99_24/12/2019 5:41:48 PM","2019-12-11","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Few railings on deck are all around bent & damaged","Miscellaneous","Structural Condn. / WT integrity ","External Factors",11.3,"Medium","Not Applicable","Not Applicable","Need to fabricate & Renew","2020-12-30",null,"Deferred to D D",null,"Yes","No","No","Internal"]
[null,null,null,null,9038,"99_24/12/2019 6:00:03 PM","2019-12-11","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Both the gangway Inclinometer Missing","Miscellaneous","General Appearance","Equipment Related",5.47,"Medium","Not Applicable","Not Applicable","New gangway angle indicator need to be fixed. GANGWAY ANGLE INDICATOR ORDERED","2020-06-30","PERF200053","Not Started",null,"No","No","No","Internal"]
[null,null,null,null,9039,"99_24/12/2019 5:25:33 PM","2019-12-11","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Luboil manifold containment tray observed to be corroded from edges","Miscellaneous","Structural Condn. / WT integrity ","Equipment Related",6.9,null,"Not Applicable","Not Applicable","Need to fabricate &  Renew","2020-12-30",null,"Deferred to D D",null,"Yes","No","No","Internal"]
[null,null,null,null,null,"99_9/1/2020 9:27:38 PM","2019-11-29","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ME Shaft power meter not operational.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related",null,null,"Not Applicable","Not Applicable","shore technician to service and make the system operational.","2020-02-29",null,"Not Started",null,"No",null,null,"Internal"]
[null,null,null,null,null,"99_27/02/2020 11:05:34","2020-01-17","Defect","Ship Staff","Ship Staff Insp.","AUX ENGINE fuel oil system outlet pressure regualting valve not operating as required. ","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Pressure regulating valve need to be renewed/overhauled.","2020-04-17","PERF200010 -  G/E F.O PRESSURE REGULATING VALVE","Waiting spare",null,"No",null,null,"Internal"]
[null,null,null,null,null,"99_28/2/2020 2:44:33 PM","2019-12-11","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Both Windlass Hydraulic Brakes In operational through brake lever, Brake cylinder leaking, Hydraulic brake lever Freezed. Presently Vessel is using Brakes by manual operation","Deck - Mooring Machinery","Mooring","Equipment Related",9.1999999999999993,"Very High","Not Applicable","Not Applicable","NEED TO RENEW / OVERHAUL","2020-06-30",null,"Not Started",null,"No",null,null,"Internal"]
[null,null,null,null,null,"99_8/3/2020 5:09:20 PM","2020-03-03","Defect","Ship Staff","Ship Staff Insp.","Port provision crane ladder safety hoop ( railing )found broken from weld part","Deck - Machinery","General Appearance","Equipment Related",null,null,"Not Applicable","Not Applicable","Cold work completed","2020-12-30",null,"Deferred to D D",null,"No",null,null,"Internal"]
[null,null,null,null,null,"99_8/3/2020 5:11:24 PM","2020-02-29","Defect","Ship Staff","Ship Staff Insp.","Both lifeboat self lowering wire winch drum found wasted & holed.","LSA / FFA","LSA / FFA Appliances","Equipment Related",5.29,"High","Not Applicable","Not Applicable","Need to fabricate & Renew","2020-07-30",null,"Not Started",null,"No",null,null,"Internal"]
[null,null,null,null,null,"99_21/3/2020 3:22:58 PM","2020-03-06","Defect","Ship Staff","Ship Staff Insp.","Fwd Mast 3-4 Ladder Rungs Rusted & Thinned down","Miscellaneous","General Appearance","Inappropriate Procedure",null,"Low","Not Applicable","Not Applicable","Need to fabricate","2020-12-30",null,"Deferred to D D",null,"No",null,null,"Internal"]
[null,null,null,null,null,"99_21/3/2020 3:32:39 PM","2020-03-15","Defect","Ship Staff","Ship Staff Insp.","Pressure Guage for IG System on deck, Pumproom top, CCR, Bridge showing different pressure readings","Inert Gas","Cargo / Ballast Systems","Equipment Related",8.1300000000000008,"Medium","Not Applicable","Not Applicable","Need to to Calibrate","2020-07-15",null,"Not Started",null,"No",null,null,"Internal"]
[null,null,null,null,null,"99_21/3/2020 3:34:38 PM","2020-03-15","Defect","Ship Staff","Ship Staff Insp.","Tank Cleaning heater temperature guage /& Pressure Transmitter on deck in operational","Miscellaneous","Cargo / Ballast Systems","Equipment Related",8.1300000000000008,"Medium","Not Applicable","Not Applicable","Troubleshooting in progress","2020-07-15",null,"In progress",null,"No",null,null,"Internal"]
[null,null,null,null,null,"99_22/3/2020 1:13:07 PM","2020-03-22","Defect","Ship Staff","Ship Staff Insp.","Aircon outlet dispenser missing in 3-4  cabins ","Accommodation ","MLC Related","Inappropriate Procedure",null,null,"Not Applicable","Not Applicable","Need to fabricate or renew","2020-06-30",null,"Not Started",null,"No",null,null,"Internal"]
[null,null,null,null,null,"99_22/3/2020 11:19:43 PM","2020-02-13","Defect","Ship Staff","Ship Staff Insp.","Stbd side Bridge Wing Fire Box Holding Arrangement wasted need to fabricate.","LSA / FFA","LSA / FFA Appliances","Inappropriate Procedure",null,null,"Not Applicable","Not Applicable","Need to fabricate.","2020-07-13",null,"Not Started",null,"No",null,null,"Internal"]
[null,null,null,null,null,"99_24/3/2020 1:24:03 AM","2020-01-25","Defect","Ship Staff","Ship Staff Insp.","Port side bridge wing sound reception system mic not working","Navigation - Others","Navigation","Equipment Related",4.7,"High","Not Applicable","Not Applicable","Spare recieved, to be renewed","2020-07-01","PERF200027","In progress",null,"No",null,null,"Internal"]
[null,null,null,null,null,"99_25/3/2020 1:05:00 PM","2020-03-23","Defect","Ship Staff","Ship Staff Insp.","1w, 2w, 4w Ballast tank sounding pipes on deck are fully corroded. also the threads for putting sounding caps in pipe is fully corroded, resulting in the caps are not going & fitting on sounding pipe","Miscellaneous","Structural Condn. / WT integrity ","Inappropriate Procedure",11.4,"Very High","Not Applicable","Not Applicable","TEMPORARY REPAIRS CARRIED OUT","2020-12-30",null,"Deferred to D D",null,"No",null,null,"Internal"]
[null,null,null,null,null,"99_25/3/2020 1:19:35 PM","2020-03-25","Defect","Ship Staff","Ship Staff Insp.","Both Slop tanks heating coils are heavily rusted & wasted / holed in cargo tanks. after checking on deck.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related",11.4,"Very High","Not Applicable","Not Applicable","Need fabrication & renewal","2020-12-30",null,"Deferred to D D",null,"No",null,null,"Internal"]
[null,null,null,null,null,"99_26/03/2020 03:15:03","2020-02-20","Defect","Ship Staff","Ship Staff Insp.","Low Sea chest filter inlet valve cannot be operated manually due the Damaged Worm gear teeth. Also the worm gear is heavly rusted and jammed on the shaft.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related",10.3,"Medium","Not Applicable","Not Applicable","Low sea chest manual operation vavle gear box gear to be removed and gear box to be renewed.","2020-12-20","PERF200127","Deferred to D D",null,"Yes",null,null,"Internal"]
[null,null,null,null,null,"99_27/3/2020 1:05:38 AM","2019-11-28","Defect","Ship Staff","Ship Staff Insp.","HDM display on steering stand flickering & unreadable ","Navigation - Others","Navigation","Equipment Related",4.7,"High","Not Applicable","Not Applicable","RO raised, awaiting spare","2020-07-01","PERF200030","Waiting spare",null,"No",null,null,"Internal"]
[null,null,null,null,null,"99_27/3/2020 1:14:12 AM","2019-11-28","Defect","Ship Staff","Ship Staff Insp.","Both bridge wing RPM indicator markings faded ","Navigation - Others","Navigation","Equipment Related",4.7,"High","Not Applicable","Not Applicable","Both repeaters were opened & markings were highlighted with permanent marker. Both repeaters to be renewed at next drydock.","2020-12-01",null,"Deferred to D D",null,"No",null,null,"Internal"]
[null,null,null,null,null,"99_27/03/2020 06:09:47","2020-02-28","Defect","Ship Staff","Ship Staff Insp.","THREADS OF SOUNDING PIPE OF OILY BILGE TANK NOT IN GOOD CONDITION.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Inappropriate Procedure",10.3,"Medium","Not Applicable","Not Applicable","SOUNDING PIPE HEAD TO BE RENEWED.","2020-05-28","PERF200101","Waiting spare",null,"No",null,null,"Internal"]
[null,null,null,null,null,"99_27/03/2020 13:45:51","2020-03-25","Defect","Ship Staff","Ship Staff Insp.","Main Engine turning gear gear box oil leaking from shaft seal.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related",10.3,"Medium","Not Applicable","Not Applicable","M.E turning gear gear box shaft seal need to be renewed.","2020-11-30",null,"Deferred to D D",null,"Yes",null,null,"Internal"]
[null,null,null,null,null,"99_08/04/2020 18:45:23","2020-02-05","Defect","Ship Staff","Ship Staff Insp.","AIR EJECTOR CONDENSER 20% INLET SIDE TUBES FOUND ERRODED AND 7 TUBES PLUGED. ","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related",10.3,"Medium","Not Applicable","Not Applicable","AIR EJECTOR NEED TO BE REPLACED/TUBES RENEWED.","2020-05-05","PERF200044","Waiting spare",null,"No",null,null,"Internal"]
[null,null,null,null,null,"99_10/4/2020 6:50:34 PM","2020-03-25","Defect","Ship Staff","Ship Staff Insp.","Casing of Two Engine room blowers Fwd side P & S found wasted & holed from many places","Miscellaneous","General Appearance","Equipment Related",null,null,"Not Applicable","Not Applicable","Temporary repairs carried out. Fabrication need to be carried out in dry dock","2020-12-30",null,"Deferred to D D",null,"No",null,null,"Internal"]
[null,null,null,null,null,"99_13/04/2020 01:05:03","2020-03-02","Defect","Ship Staff","Ship Staff Insp.","M.E Air cooler air side gaskets leaking.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related",10.34,"High","Not Applicable","Not Applicable","M.E Air cooler air side gaskets need to be renewed.","2020-12-01",null,"Deferred to D D",null,"Yes",null,null,"Internal"]
[null,null,null,null,null,"99_14/4/2020 7:30:57 PM","2020-02-20","Defect","Ship Staff","Ship Staff Insp.","Two portable gas meters sensor cartridge expired. ","Miscellaneous","ISM Related","Equipment Related",5.23,"Very High","Not Applicable","Not Applicable","RO Raised. Awaiting spares","2020-07-30","PERF200061","Waiting spare",null,"No",null,null,"Internal"]
[null,null,null,null,null,"99_14/4/2020 7:39:36 PM","2020-03-11","Defect","Ship Staff","Ship Staff Insp.","Hydraulic leaks are there in cargo tanks. ","Cargo Mach.","Cargo / Ballast Systems","Equipment Related",11.4,"Very High","Not Applicable","Not Applicable","Need to check the leaks after going in tanks. & then can make more exact assesment of the leaks.","2020-06-15",null,"Not Started",null,"No",null,null,"Internal"]
[null,null,null,null,null,"99_15/4/2020 8:32:39 PM","2020-04-13","Defect","Ship Staff","Ship Staff Insp.","Both Vapour line port & stbd Fwd ones have a soft patch near drain line near vapour line blank","Inert Gas","Cargo / Ballast Systems","Equipment Related",11.4,"Very High","Not Applicable","Not Applicable","Cold work carried out.","2020-12-30",null,"Deferred to D D",null,"No",null,null,"Internal"]
[null,null,null,null,null,"99_16/4/2020 3:55:36 PM","2020-04-02","Defect","Ship Staff","Ship Staff Insp.","FPK Tank remote sounding guage showing error","Miscellaneous","Cargo / Ballast Systems","Equipment Related",null,null,"Not Applicable","Not Applicable"," Level sensor need to be renewed","2020-06-30","PERF205026","Waiting spare",null,"No",null,null,"Internal"]
[null,null,null,null,null,"99_17/4/2020 1:01:56 PM","2020-04-01","Defect","Ship Staff","Ship Staff Insp.","SAAB Tank radar tank domes inspection hatch cover are heavily rusted & wasted condition","Miscellaneous","General Appearance","Equipment Related",11.3,"Medium","Not Applicable","Not Applicable","Need to be fabricated & renewed in Drydock","2020-12-30",null,"Deferred to D D",null,"No",null,null,"Internal"]
[null,null,null,null,null,"99_17/4/2020 1:39:22 PM","2020-04-01","Defect","Ship Staff","Ship Staff Insp.","Sbbd Manifold dip tray lip is wasted & holed from many places.","Miscellaneous","Cargo / Ballast Systems","Equipment Related",6.6,"Medium","Not Applicable","Not Applicable","Cold work carried out. Need to fabricate in dry dock","2020-12-30",null,"Deferred to D D",null,"No",null,null,"Internal"]
[null,null,null,null,null,"99_30/04/2020 17:56:33","2020-04-21","Defect","Ship Staff","Ship Staff Insp.","IG deck seal pump # 1 & 2 discharge valve not holding the pressure.\t","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related",10.3,"Medium","Not Applicable","Not Applicable","IG deck seal pump # 1 & 2 discharge valve need to be renewed. Kindly note Maintenance jobs on pump can be done by stopping both the pumps and draining the line.","2020-07-21","PERF200142","Waiting spare",null,"No",null,null,"Internal"]
[null,null,null,null,null,"99_30/04/2020 18:04:23","2020-04-25","Breakdown","Ship Staff","Ship Staff Insp.","Deck air compressor Driving belts broken.","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related",10.3,"High","Not Applicable","Not Applicable","Deck air compressor Driving belts to be renewed.","2020-06-25","PERF200133","Waiting spare",null,"No",null,null,"Internal"]
[null,null,null,null,null,"99_15/05/2020 10:09:31","2020-04-11","Observation,Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Engine casing area is dirty. Same to be upgraded.","Miscellaneous","Eng. / Strg. Comp.","External Factors",null,null,"Not Applicable","Not Applicable","Engine room casing area cleaning and painting in progress.","2020-07-11",null,"In progress",null,"No",null,null,"Internal"]
[null,null,null,null,null,"99_17/5/2020 12:21:43 PM","2020-04-11","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Name forward/ Aft to be re stencilled at next suitable anchorage. ","Miscellaneous","General Appearance","Inappropriate Procedure",11.2,"Medium","Not Applicable","Not Applicable","Need to stencill Again","2020-07-15",null,"Not Started",null,"No",null,null,"Internal"]
[null,null,null,null,null,"99_17/5/2020 12:26:49 PM","2020-04-11","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Some areas fwd of midship are in very poor condition. Same to be attended on priority.","Deck - Pipe / Fittings","General Appearance","Inappropriate Procedure",11.2,"Medium","Not Applicable","Not Applicable","Derusting & painting in progress","2020-07-15",null,"In progress",null,"No",null,null,"Internal"]
[null,null,null,null,null,"99_17/5/2020 12:28:32 PM","2020-04-11","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Paint peel off on Main deck especially on the stbd side to be hydro blasted and repainted. ","Deck - Pipe / Fittings","General Appearance","Inappropriate Procedure",11.2,"Medium","Not Applicable","Not Applicable","Derusting & painting in progress","2020-07-15",null,"In progress",null,"No",null,null,"Internal"]
[null,null,null,null,null,"99_17/5/2020 12:31:46 PM","2020-04-11","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Rusted U Bolts on main deck require renewal","Deck - Pipe / Fittings","General Appearance","Equipment Related",11.5,"Medium","Not Applicable","Not Applicable","Renewal in progress","2020-07-15",null,"In progress",null,"No",null,null,"Internal"]
[null,null,null,null,null,"99_17/5/2020 12:37:47 PM","2020-04-11","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Pump Room blowers to be de rusted and painted","Miscellaneous","General Appearance","Inappropriate Procedure",11.8,"Low","Not Applicable","Not Applicable","Need to derust & paint","2020-06-11",null,"In progress",null,"No",null,null,"Internal"]
[null,null,null,null,null,"99_17/5/2020 12:40:03 PM","2020-04-11","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Cow lines and IG Valves require maintenance","Deck - Pipe / Fittings","General Appearance","Inappropriate Procedure",11.4,"Very High","Not Applicable","Not Applicable","Need to derust the pipelines, U clamps to renew. IG Valves need to derust & paint","2020-06-30",null,"In progress",null,"No",null,null,"Internal"]
[null,null,null,null,null,"99_17/5/2020 12:44:03 PM","2020-04-11","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Some of the PV Valves are leaking. To be overhauled. ","Inert Gas","Cargo / Ballast Systems","Equipment Related",8.19,null,"Not Applicable","Not Applicable","Need to overhaul","2020-07-15","PERF200120","Waiting spare",null,"No",null,null,"Internal"]
[null,null,null,null,null,"99_17/5/2020 12:45:38 PM","2020-04-11","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Accommodation block requires painting. ","Miscellaneous","General Appearance","Inappropriate Procedure",11.8,"Low","Not Applicable","Not Applicable","Derusting & painting in progress.","2020-07-15",null,"In progress",null,"No",null,null,"Internal"]
[null,null,null,null,null,"99_18/5/2020 1:47:00 PM","2020-04-24","Defect","Ship Staff","Ship Staff Insp.","No.2 Ballast pump suction valve BA 032 actuator leaking while opening side the valve","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related",8.11,"Medium","Not Applicable","Not Applicable","Oil seal need to be renewed","2020-07-15","PER200163","Waiting spare",null,"No",null,null,"Internal"]
[null,null,null,null,null,"99_31/05/2020 09:02:07","2020-05-15","Breakdown,Defect","Ship Staff","Ship Staff Insp.","COPT # 3 tripped during discharge operation.","Cargo Mach.","Eng. / Strg. Comp.","Equipment Related",null,null,"Not Applicable","Not Applicable","COPT # 3 trouble shooting carried out, found Over Speed Trip relay was malfunctioning. Same ordered.","2020-07-15","PERF200168 -- CARGO PUMP TURBINE RELAY","Waiting spare",null,"No",null,null,"Internal"]
[null,null,null,null,null,"99_9/6/2020 5:24:14 PM","2020-06-01","Defect","Ship Staff","Ship Staff Insp.","Stripping pump stroke counter not fucntioning properly","Cargo Mach.","Cargo / Ballast Systems","Equipment Related",8.8000000000000007,null,"Not Applicable","Not Applicable","Trouble shooting in progress.","2020-07-30",null,"In progress",null,"No",null,null,"Internal"]
[null,null,null,null,null,"99_12/6/2020 3:18:43 PM","2020-06-10","Defect","Ship Staff","Ship Staff Insp.","No.8 Foam monitor nozzle found cracked & broken","LSA / FFA","LSA / FFA Appliances","Equipment Related",5.38,"High","Not Applicable","Not Applicable","Need to Renew / Fabricate","2020-11-30",null,"Deferred to D D",null,"No",null,null,"Internal"]
[null,null,null,null,null,"99_12/06/2020 17:24:31","2020-06-07","Defect","Ship Staff","Ship Staff Insp.","Control air Dryer operation not satisfactory.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related",10.34,"High","Not Applicable","Not Applicable","Control air dryer Trouble shooting to be carried out.","2020-08-07",null,"In progress",null,"No",null,null,"Internal"]
[null,null,null,null,null,"99_12/06/2020 17:30:06","2020-04-07","Breakdown,Defect","Ship Staff","Ship Staff Insp.","Ref system recovery compressor not operational.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related",null,null,"Not Applicable","Not Applicable","Recovery comp. R.O raised.","2020-07-07","PERF200091","Waiting spare",null,"No",null,null,"Internal"]
[null,null,null,null,null,"99_12/06/2020 17:34:15","2020-04-03","Defect","Ship Staff","Ship Staff Insp.","F.W.G ejector pump small leak from Filter top cover.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related",null,null,"Not Applicable","Not Applicable","FWG ejector pump Filter body need to be renewed as the sealing surface is not in good condition.","2020-07-03",null,"In progress",null,"No",null,null,"Internal"]

{"sheet":"Completed","index":1,"n_rows":246,"n_cols":28,"rows_kept":246,"cut":false,"hidden":false,"merged":[[10,8,10,9],[10,12,10,13],[12,6,12,27],[8,6,8,27]]}
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,"Defect - Damage Monitoring Sheet"]
[]
[null,null,null,null,null,null,null,"Date of Report","31-11-2019",null,null,"Ship Name","PERFECT (26-12-2019)"]
[]
[null,null,null,null,null,null,"VERSION : 2.0"]
[]
[]
[]
[null,null,null,null,"ID","UNIQUE ID","Date Recorded","Type of Deficiency","Observer code","Type of Inspection","Description of Deficiency","Equipment Categories","Area of Observation","Deficiency Cause","VIQ Ref Number","Risk Value of Obs","PSC Ref Number","PSC MOU ID","Action Taken or Required","Target Date","PO Ref No.","Status Code","Date Completed","Drydock","Info Sharing","Critical Item","Audit Type","Superintendent Remarks"]
[null,null,null,null,8976,"99_20/12/2019 8:52:45 PM","2019-11-27","Defect","Ship Staff","Ship Staff Insp.","Boiler no.1 Main steam stop valve leaking from the bonnet","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","boiler isolated depressurized and bonnet gasket renewed.","2019-12-15","","Completed","2019-12-09","No","No","No","Internal"]
[null,null,null,null,8977,"99_20/12/2019 9:23:33 PM","2019-11-29","Defect","Ship Staff","Ship Staff Insp.","A.E 1 Fuel filter leaking","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","fuel filter isolated o ring replaced and leak rectified","2019-12-10","","Completed","2019-12-10","No","No","No","Internal"]
[null,null,null,null,8978,"99_20/12/2019 9:28:43 PM","2019-11-27","Defect","Ship Staff","Ship Staff Insp.","UNIT NO3 and 5 TOP piston ring but found to be broken ","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","piston Overhaul carried out and piston rings replaced with new spares.","2019-12-15","","Completed","2019-12-11","No","No","No","Internal"]
[null,null,null,null,8979,"99_21/12/2019 4:39:19 PM","2019-11-26","Breakdown","Ship Staff","Others (Eg. Insurance etc.)","MAIN AIR COMP # 2 COUPLING JAWS AND SPIDER WERE BROKEN.","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related","","","","","MAC # 2 BOTH MOTOR AND COMPRESSIR SIDE COUPLING AND SPIDER RENEWED.","2019-11-30","","Completed","2019-11-27","No","No","No","External"]
[null,null,null,null,8980,"99_21/12/2019 5:01:34 PM","2019-12-10","Breakdown","Ship Staff","Ship Staff Insp.","EXHAUST GAS ECONOMISER WATER INLET VALVE LEAKING FROM BONNET.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","EGB DRAINED &  DEPRESSURIZED, VALVE BONNET GASKET RENEWED. ","2019-12-11","","Completed","2019-12-10","No","No","No","Internal"]
[null,null,null,null,8981,"99_21/12/2019 5:06:41 PM","2019-12-17","Breakdown","Ship Staff","Ship Staff Insp.","HFO PURIFIER # 2 LEAKING FROM WATER SIDE.","E/R - Purifier","Eng. / Strg. Comp.","Equipment Related","","","","","HFO PURIFER # 2 SEALING WATER SOLENOID VALVE DIAPHRAGM RENEWED AS WAS NOT IN GOOD CONDITION.","2019-12-18","","Completed","2019-12-17","No","No","No","Internal"]
[null,null,null,null,8982,"99_21/12/2019 5:10:04 PM","2019-12-18","Breakdown","Ship Staff","Ship Staff Insp.","STEERING GEAR GREASING PUMP PRESSURE GAUGE NOT WORKING.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","STEERING GEAR GREASING PUMP PRESSURE GAUGE RENEWED.","2019-12-20","","Completed","2019-12-18","No","No","No","Internal"]
[null,null,null,null,8983,"99_21/12/2019 5:13:27 PM","2019-12-13","Other","Ship Staff","Ship Staff Insp.","ENGINE ROOM TOILET DRAIN FOUND CHOCK.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","ENGINE ROOM TOILET DRAIN PIPE REMOVED AND CLEARED. ","2020-01-13","","Completed","2019-12-18","No","No","No","Internal"]
[null,null,null,null,8984,"99_21/12/2019 5:29:36 PM","2019-12-05","Breakdown","Ship Staff","Ship Staff Insp.","BOILER # 2 IGNITION TRANSFORMER NOT OPERATIONAL.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","BOILER # 2 IGNITION TRANSFORMER RELACED WITH NEW SPARE TRANSFORMER. BOILER TRIED OUT, FOUND WORKING FINE.","2020-01-05","","Completed","2019-12-16","No","No","No","Internal"]
[null,null,null,null,8985,"99_23/12/2019 10:57:48 PM","2019-12-11","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Safety guard for grinder disconnected","Miscellaneous","General Appearance","Human Error","","","","","Guards put back /  Renewed","2019-12-30","","Completed","2019-12-15","No","No","No","Internal"]
[null,null,null,null,8986,"99_23/12/2019 12:48:41 PM","2019-11-27","Defect","Ship Staff","Ship Staff Insp.","ALL PV VALVES FLAME SCREENS FOUND WASTED","Cargo Mach.","Cargo / Ballast Systems","Equipment Related",11.7,"High","Not Applicable","Not Applicable","ALL PV VALVES FLAME SCREEN RENEWED","2019-12-20",null,"Completed","2019-12-07","No","No","No","Internal"]
[null,null,null,null,8987,"99_23/12/2019 10:28:14 PM","2019-11-27","Defect","Ship Staff","Ship Staff Insp.","BOTH HOSE HANDLING CRANE VALVE BLOCK FOUND WASTED. ALSO VARIOUS FITTINGS & HYDRAULIC HOSES FOUND WASTED","Deck - Machinery","General Appearance","Equipment Related",8.5,"Medium","Not Applicable","Not Applicable","BOTH CRANES VALVE BLOCK RENEWED. ALSO VARIOUS FITTINGS RENEWED","2019-12-30",null,"Completed","2019-12-11","No","No","No","Internal"]
[null,null,null,null,8988,"99_23/12/2019 10:31:53 PM","2019-11-27","Defect","Ship Staff","Ship Staff Insp.","CREW PANTRY DISH WASHER IN OPERATIONAL","Miscellaneous","MLC Related","Equipment Related",11.16,"Low","Not Applicable","Not Applicable","NEW DISH WASHER REPLACED.","2020-01-30",null,"Completed","2019-12-15","No","No","No","Internal"]
[null,null,null,null,8989,"99_23/12/2019 10:50:18 PM","2019-12-11","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Needle guns & Grinder on deck were observed with activating lever secured with seizing wires","Miscellaneous","General Appearance","Human Error","","","","","ALL NEEDLE GUNS ACTIVATING LEVER FREED, ","2019-12-30","","Completed","2019-12-14","No","No","No","Internal"]
[null,null,null,null,8990,"99_23/12/2019 10:37:51 PM","2019-11-27","Defect","Ship Staff","Ship Staff Insp.","COW LINE PRESSURE GUAGE IN CCR NOT OPERATIONAL","Cargo Mach.,Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related",8.1300000000000008,"Medium","Not Applicable","Not Applicable","CCR GUAGE CALIBERATED BY SHORE TECHNICIAN. NOW WORKING NORMAL","2019-12-30",null,"Completed","2019-12-11","No","No","No","Internal"]
[null,null,null,null,8991,"99_23/12/2019 10:09:38 PM","2019-11-27","Defect","Ship Staff","Ship Staff Insp.","FWD COW LINE PRESSURE GUAGE NOT READABLE","Deck - Pipe / Fittings","Cargo / Ballast Systems","Inappropriate Procedure",8.1300000000000008,"Medium","Not Applicable","Not Applicable","PRESSURE GUAGE RENEWED","2019-12-30",null,"Completed","2019-12-24","No","No","No","Internal"]
[null,null,null,null,8992,"99_23/12/2019 10:14:30 PM","2019-11-27","Defect","Ship Staff","Ship Staff Insp.","78 NOS of foam extinguisher gas catridges expiring on dec 2019","LSA / FFA","LSA / FFA Appliances","Equipment Related","","","","","All Foam extinguishergas cartridges renewed.","2019-12-30","","Completed","2019-12-11","No","No","No","Internal"]
[null,null,null,null,8993,"99_24/12/2019 12:10:27 PM","2019-12-11","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","NAME TAG OF LIFERAFT TO BE UPDATED","LSA / FFA","LSA / FFA Appliances","Inappropriate Procedure","","","","","UPDATED & COMPLETED","2019-12-30","","Completed","2019-12-13","No","No","No","Internal"]
[null,null,null,null,8994,"99_24/12/2019 12:23:16 PM","2019-12-11","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","EYE PROTECTION IN PAINT LOCKER FOUND BROKEN","Miscellaneous","General Appearance","Inappropriate Procedure","","","","","RENEWED","2019-12-20","","Completed","2019-12-13","No","No","No","Internal"]
[null,null,null,null,8995,"99_24/12/2019 2:03:35 PM","2019-12-10","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","All computer cables to be arranged properly and secure all computers.All LAN cables, network switch, power cables to be secured and lay up properly at all location","Navigation - Others","Communication","Equipment Related","","","","","cables arranged and secured","2019-12-25","","Completed","2019-12-22","No","No","No","Internal"]
[null,null,null,null,8996,"99_24/12/2019 2:07:10 PM","2019-12-10","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Bridge- a) All All unncesseary cables to be removed from all places and secured all necessary cables properly.","Navigation - Others","Communication","Equipment Related","","","","","unncessary cables removed and ,all cables secured.","2019-12-17","","Completed","2019-12-16","No","No","No","Internal"]
[null,null,null,null,8997,"99_24/12/2019 4:04:22 PM","2019-12-11","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","LIFEBUOY GRAB LINES NEEDS RENEWAL","LSA / FFA","LSA / FFA Appliances","Inappropriate Procedure",5.31,"High","Not Applicable","Not Applicable","ALL LIFEBUOYS GRAB LINE RENEWED","2020-01-30",null,"Completed","2019-12-20","No","No","No","Internal"]
[null,null,null,null,8998,"99_24/12/2019 4:29:15 PM","2019-12-11","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Ships name stencilled on OARS inside both lifeboats to be changed","LSA / FFA","LSA / FFA Appliances","Inappropriate Procedure","","","","","Old Ship name Stencilled removed","2019-12-30","","Completed","2019-12-23","No","No","No","Internal"]
[null,null,null,null,8999,"99_24/12/2019 4:58:06 PM","2019-12-11","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Vessel not equipped with one or two carbon dioxide extinguishers with total capacity of not more than 18 kg as required by 4.7 of guide to helicopter operations & SOLAS chap- II-2 regulation 18, However spare CO2 extinguishers are considered as a substitute for same.","LSA / FFA","LSA / FFA Appliances","Inappropriate Procedure","","","","","New extinguisher received & stored in location","2019-12-30","","Completed","2019-12-12","No","No","No","Internal"]
[null,null,null,null,9000,"99_24/12/2019 5:01:36 PM","2019-12-11","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Emergency Stop’ IMO symbol to be pasted near AE Emergency shut off valves","E/R - Aux. Engine","Emgcy. Systems","Inappropriate Procedure","","","","","New IMO Symbols pasted","2019-12-30","","Completed","2019-12-15","No","No","No","Internal"]
[null,null,null,null,9001,"99_24/12/2019 5:12:22 PM","2019-12-11","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Port lifeboat bilge pipe to be freed","LSA / FFA","LSA / FFA Appliances","Inappropriate Procedure","","","","","Bilge pump pipe freed","2019-12-30","","Completed","2019-12-14","No","No","No","Internal"]
[null,null,null,null,9002,"99_24/12/2019 5:19:57 PM","2019-12-11","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Wooden planks on top of battery box inside both lifeboat to be secured back in place","LSA / FFA","LSA / FFA Appliances","Inappropriate Procedure","","","","","All the covers secured back in place","2019-12-30","","Completed","2019-12-14","No","No","No","Internal"]
[null,null,null,null,9003,"99_24/12/2019 5:28:43 PM","2019-12-11","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Butterfly nuts for box of sludge emergency stop to be freed & greased","Miscellaneous","Emgcy. Systems","Inappropriate Procedure","","","","","All the butterfly nuts for the box greased & freed","2020-01-30","","Completed","2019-12-22","No","No","No","Internal"]
[null,null,null,null,9004,"99_24/12/2019 5:57:01 PM","2019-12-11","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","All containment trays require cleaning and the plugs to be checked for leakage and secured with wire","Miscellaneous","General Appearance","Inappropriate Procedure","","","","","All the dip trays cleaned & dip tray plugs plugged ","2019-12-30","","Completed","2019-12-20","No","No","No","Internal"]
[null,null,null,null,9005,"99_24/12/2019 5:17:10 PM","2019-12-11","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Both lifeboat steering mechanism require de-rusting","LSA / FFA","LSA / FFA Appliances","Equipment Related","","","","","Derusting & Painting completed","2020-01-20","","Completed","2019-12-24","No","No","No","Internal"]
[null,null,null,null,9006,"99_24/12/2019 9:41:18 PM","2019-12-11","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Bolts for bottom securing of forward ladder of cargo valve cross over platform were observed to be loose","Miscellaneous","Structural Condn. / WT integrity ","Inappropriate Procedure","","","","","Bolts were missing for the platform ladder, same renewed","2020-01-15","","Completed","2019-12-21","No","No","No","Internal"]
[null,null,null,null,9007,"99_24/12/2019 9:46:43 PM","2019-12-11","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Oil below hydraulic hose tray forward of no-3 COP","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","Area cleaned Thoroughly. ","2019-12-30","","Completed","2019-12-21","No","No","No","Internal"]
[null,null,null,null,9008,"99_24/12/2019 9:51:08 PM","2019-12-11","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Stbd lifeboat air flexible connections and connectors on the discharge side having minor leakage","LSA / FFA","LSA / FFA Appliances","Inappropriate Procedure","","","","","All the connections re-tighten, No leaks at present.","2019-12-25","","Completed","2019-12-24","No","No","No","Internal"]
[null,null,null,null,9009,"99_24/12/2019 10:08:43 PM","2019-12-11","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Emergency air compressor to be clearly identified and marked","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related","","","","","EMERGENCY AIR COMPRESSOR STENSILLED AND MOTOR COVER PAINTED RED.","2020-03-11","","Completed","2019-12-22","No","No","No","Internal"]
[null,null,null,null,null,"99_23/12/2019 12:44:22 PM","2019-11-27","Defect","Ship Staff","Ship Staff Insp.","VARIOUS SECTION OF VALVE HYDRAULIC LINE ON DECK FOUND WASTED","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related",11.4,"Very High","Not Applicable","Not Applicable","FABRICATION & RENEWAL  OF 18 SECTIONS OF VALVE HYDRAULIC LINE COMPLETED.","2019-12-30",null,"Completed","2019-12-28","No",null,null,"Internal"]
[null,null,null,null,null,"99_24/12/2019 4:32:12 PM","2019-12-11","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Both lifeboat davit wire requires greasing ","LSA / FFA","LSA / FFA Appliances","Equipment Related",null,null,"Not Applicable","Not Applicable","Greasing Completed","2020-01-30",null,"Completed","2019-12-24","No",null,null,"Internal"]
[null,null,null,null,null,"99_24/12/2019 4:43:48 PM","2019-12-11","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Steering gear room mush room vent stuck in position","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","Equipment Related",null,null,"Not Applicable","Not Applicable","overhauled & freed","2020-01-15",null,"Completed","2019-12-29","No",null,null,"Internal"]
[null,null,null,null,null,"99_24/12/2019 11:58:56 AM","2019-12-11","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","WIRES TURNBUCKLES HEAVILY CORRODED OF SAFETY WALKWAY & SAFE ACCESS TO TANKER BOW","Miscellaneous","General Appearance","Inappropriate Procedure",null,null,"Not Applicable","Not Applicable","DERUSTING & PAINTING COMPLETED","2020-01-15",null,"Completed","2020-01-02","No",null,null,"Internal"]
[null,null,null,null,null,"99_24/12/2019 12:04:19 PM","2019-12-11","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","PUMPROOM BILGES HAVE OIL STAINS & WATER","Miscellaneous","General Appearance","Inappropriate Procedure",null,null,"Not Applicable","Not Applicable","THOROUGHLY CLEANED","2020-01-15",null,"Completed","2019-12-30","No",null,null,"Internal"]
[null,null,null,null,null,"99_3/1/2020 9:10:20 PM","2019-12-05","Defect","Ship Staff","Ship Staff Insp.","PORT SIDE PILOT LADDER STEP FOUND BROKEN","Miscellaneous","General Appearance","Equipment Related",5.47,"Medium","Not Applicable","Not Applicable","NEW PILOT LADDER RECEIVED & RENEWED","2019-12-31",null,"Completed","2019-12-26","No",null,null,"Internal"]
[null,null,null,null,null,"99_3/1/2020 9:15:07 PM","2019-12-06","Defect","Ship Staff","Ship Staff Insp.","STBD GANGWAY HOISTING WIRE FEW STRANDS FOUND BROKEN","Miscellaneous","General Appearance","Equipment Related",null,null,"Not Applicable","Not Applicable","HOISTING WIRE RENEWED.","2020-01-15",null,"Completed","2019-12-30","No",null,null,"Internal"]
[null,null,null,null,null,"99_3/1/2020 9:17:15 PM","2019-12-12","Other","Ship Staff","Ship Staff Insp.","THREE WALKWAY PLATFORM RAMP FOUND WASTED & BROKEN","Miscellaneous","General Appearance","Inappropriate Procedure",null,null,"Not Applicable","Not Applicable","FABRICATED & RENEWED","2020-01-30",null,"Completed","2020-01-02","No",null,null,"Internal"]
[null,null,null,null,null,"99_3/1/2020 10:24:21 PM","2019-12-31","Defect","Ship Staff","Ship Staff Insp.","FOUR FRESH WATER TANK VENT HEAD COVERS FOUND WASTED","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","Inappropriate Procedure",11.7,"High","Not Applicable","Not Applicable","FABRICATED & RENEWED","2020-01-30",null,"Completed","2020-01-02","No",null,null,"Internal"]
[null,null,null,null,null,"99_3/1/2020 11:06:05 PM","2019-12-30","Defect","Ship Staff","Ship Staff Insp.","TWO APK TANK VENT HEAD COVER FOUND WASTED","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","Inappropriate Procedure",11.7,"High","Not Applicable","Not Applicable","FABRICATED & RENEWED","2020-01-30",null,"Completed","2020-01-02","No",null,null,"Internal"]
[null,null,null,null,null,"99_4/1/2020 2:53:16 AM","2019-12-31","Defect","Ship Staff","Ship Staff Insp.","Five vent head covers for ballast tank found wasted","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","Inappropriate Procedure",11.7,"High","Not Applicable","Not Applicable","Fabricated & Renewed","2020-01-30",null,"Completed","2020-01-03","No",null,null,"Internal"]
[null,null,null,null,null,"99_24/12/2019 9:43:24 PM","2019-12-11","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Stbd anchor bitter end locking pin to be freed","Miscellaneous","Emgcy. Systems","Inappropriate Procedure",9.2200000000000006,"Low","Not Applicable","Not Applicable","greased & freed","2020-01-15",null,"Completed","2020-01-03","No",null,null,"Internal"]
[null,null,null,null,null,"99_24/12/2019 4:38:38 PM","2019-12-11","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Max stowage height to be marked in paint locker & Recommend to single stack of paint","Miscellaneous","General Appearance","Inappropriate Procedure",null,null,"Not Applicable","Not Applicable","Completed","2020-01-30",null,"Completed","2020-01-04","No",null,null,"Internal"]
[null,null,null,null,null,"99_7/1/2020 2:42:54 AM","2020-01-01","Defect","Ship Staff","Ship Staff Insp.","One section of STBD Windlass Hydraulic line ( pressure side ) found wasted.","Deck - Mooring Machinery","Mooring","Equipment Related",null,null,"Not Applicable","Not Applicable","Fabricated & renewed","2020-01-15",null,"Completed","2020-01-06","No",null,null,"Internal"]
[null,null,null,null,null,"99_5/1/2020 3:40:46 AM","2020-01-03","Defect","Ship Staff","Ship Staff Insp.","Nine vent head covers for ballast tanks found wasted & holed","Deck - Pipe / Fittings","General Appearance","Inappropriate Procedure",11.7,"High","Not Applicable","Not Applicable","FABRICATED & RENEWED","2020-01-15",null,"Completed","2020-01-07","No",null,null,"Internal"]
[null,null,null,null,null,"99_7/1/2020 2:45:31 AM","2019-12-15","Defect","Ship Staff","Ship Staff Insp.","No.1 & No.3 COP & Separator drain valves suspect passing / leaking","Cargo Mach.","Cargo / Ballast Systems","Equipment Related",8.18,"High","Not Applicable","Not Applicable","TOTAL 6 VALVE RENEWED","2020-01-30",null,"Completed","2020-01-07","No",null,null,"Internal"]
[null,null,null,null,null,"99_24/12/2019 4:41:07 PM","2019-12-11","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Paying out direction for wires missing from few mooring drums","Miscellaneous","Mooring","Inappropriate Procedure",9.19,"Low","Not Applicable","Not Applicable","Stencilling & Highlighting Completed","2020-01-30",null,"Completed","2020-01-09","No",null,null,"Internal"]
[null,null,null,null,null,"99_24/12/2019 9:54:58 PM","2019-12-10","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Old Iridium antenna on stbd side bridge wing to be removed, cut the pole and secure cable properly","Navigation - GMDSS & Communication","Communication","Equipment Related",null,null,"Not Applicable","Not Applicable","REMOVED","2020-01-10",null,"Completed","2020-01-10","No",null,null,"Internal"]
[null,null,null,null,null,"99_24/12/2019 10:17:47 PM","2019-12-11","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Discharge pressure Gauges for No-1 & 2 IG deck seal pump having errors","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related",8.25,"Very High","Not Applicable","Not Applicable","pressure gauge renewed.","2020-03-11",null,"Completed","2020-01-08","No",null,null,"Internal"]
[null,null,null,null,null,"99_24/12/2019 10:27:40 PM","2019-12-11","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Secure spare impeller in air con room","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related",5.1100000000000003,"Low","Not Applicable","Not Applicable","Spare impeller secured","2020-03-11",null,"Completed","2019-12-22","No",null,null,"Internal"]
[null,null,null,null,null,"99_23/12/2019 8:10:03 PM","2019-12-11","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Spool piece for E/RM sludge to slop transfer to be clearly identified and marked","Deck - Pipe / Fittings","MARPOL Related","Equipment Related",2.11,"Medium","Not Applicable","Not Applicable","Spool piece painted, stencilled & secured.","2020-03-11",null,"Completed","2020-01-08","No",null,null,"Internal"]
[null,null,null,null,null,"99_23/12/2019 8:14:00 PM","2019-12-11","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Safety guard missing from follow pumps – No-1 FW hydrophore pump, FW ejector pump, No-1,2,3 C.S.W pump, Scrubber pump, No-1&2 fire & G.S pump","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related",10.27,"Medium","Not Applicable","Not Applicable","SAFETY GUARDS FABRICATED AND PUT.","2020-03-11",null,"Completed","2020-01-07","No",null,null,"Internal"]
[null,null,null,null,null,"99_23-12-2019 13:06:00","2019-12-11","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","FWG ejector pump discharge valve leaking from bonnet","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related",10.3,"Medium","Not Applicable","Not Applicable","FWG Ejector pump discharge valve bonnet gasket renewed.","2020-03-11",null,"Completed","2020-01-13","No",null,null,"Internal"]
[null,null,null,null,null,"99_27/02/2020 06:05:09","2019-12-11","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Engine room toilet door to be fitted back in place properly","Miscellaneous","Eng. / Strg. Comp.","Inappropriate Procedure",null,null,"Not Applicable","Not Applicable","Engine room toilet door hinge pin was missing, Same fabricated & put back","2020-03-11",null,"Completed","2020-01-17","No",null,null,"Internal"]
[null,null,null,null,null,"99_27/02/2020 06:34:12","2019-12-11","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Discharge pressure Gauges for No-1 & 2 IG deck seal pump having errors","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Discharge pressure Gauges for No-1 & 2 IG deck seal pump renewed","2020-03-11",null,"Completed","2020-01-08","No",null,null,"Internal"]
[null,null,null,null,null,"99_27/02/2020 06:37:23","2019-12-13","Defect","Ship Staff","Ship Staff Insp.","ENGINE ROOM TOILET DRAIN FOUND CHOCK.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related",null,null,"Not Applicable","Not Applicable","ENGINE ROOM TOILET DRAIN PIPE REMOVED AND CLEARED.","2020-01-13",null,"Completed","2019-12-18","No",null,null,"Internal"]
[null,null,null,null,null,"99_27/02/2020 06:43:27","2019-12-17","Breakdown","Ship Staff","Ship Staff Insp.","HFO PURIFIER # 2 F.O SATARTED LEAKING FROM WATER SIDE DURING OPERATION.","E/R - Purifier","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","HFO PURIFER # 2 SEALING WATER SOLENOID VALVE DIAPHRAGM RENEWED AS WAS NOT IN GOOD CONDITION.","2020-01-18",null,"Completed","2019-12-17","No",null,null,"Internal"]
[null,null,null,null,null,"99_27/02/2020 06:46:58","2019-12-18","Defect","Ship Staff","Ship Staff Insp.","STEERING GEAR GREASING PUMP PRESSURE GAUGE NOT WORKING.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related",null,null,"Not Applicable","Not Applicable","STEERING GEAR GREASING PUMP PRESSURE GAUGE RENEWED","2019-12-20",null,"Completed","2019-12-18","No",null,null,"Internal"]
[null,null,null,null,null,"99_27/02/2020 06:49:17","2019-12-30","Breakdown","Ship Staff","Ship Staff Insp.","Boiler No. 2 pilot burner not firing due to no output from ignition transformer.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Boiler No. 2 ignition transformer renewed, Boiler tried out found working satisfactorly.","2020-01-10",null,"Completed","2020-01-02","No",null,null,"Internal"]
[null,null,null,null,null,"99_27/02/2020 08:07:17","2020-01-02","Breakdown","Ship Staff","Ship Staff Insp.","FWG ejector pump discharge side sacrificial flange and sacrificial flange before overboard valve leaking from tell tail holes.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related",10.29,"Medium","Not Applicable","Not Applicable","FWG ejector pump both inlet and outlet sacrificial flange and sacrificial flange before overboard valve renewed.","2020-03-02",null,"Completed","2020-01-11","No",null,null,"Internal"]
[null,null,null,null,null,"99_27/02/2020 08:10:27","2020-01-02","Breakdown","Ship Staff","Ship Staff Insp.","Control air compressor running at very low capacity not pressing up to required pressure.","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related",null,null,"Not Applicable","Not Applicable","Control air compressor suction valve overhauled. All Seal rings renewed. Valve put back, compressor tried out, working satisfactorly.","2020-01-03",null,"Completed","2020-01-10","No",null,null,"Internal"]
[null,null,null,null,null,"99_27/02/2020 08:13:30","2020-01-10","Breakdown","Ship Staff","Ship Staff Insp.","Boiler # 1 Valve spindle found broken of water level control valve (Big) as water level was not maintianing.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Boiler # 1 Valve spindle welded with new stud and machined. Valve spindle put back in use, found working satisfactorly.","2020-01-10",null,"Completed","2020-01-11","No",null,null,"Internal"]
[null,null,null,null,null,"99_27/02/2020 08:16:43","2020-01-15","Defect","Ship Staff","Ship Staff Insp.","Air conditioning compressor # 2 Leaking from mechanical seal.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related",10.29,"Medium","Not Applicable","Not Applicable","Air Con compressor # 2 mechanical seal & discharge valve gland O-ring renewed.","2020-02-15",null,"Completed","2020-01-21","No",null,null,"Internal"]
[null,null,null,null,null,"99_27/02/2020 08:19:04","2020-01-16","Defect","Ship Staff","Ship Staff Insp.","Boiler # 2 water drum manhole gasket leaking.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Boiler # 2 water drained, Manhole cover removed & gasket renewed. Same time steam drum manhole gasket also renewed. Also steam & water drum inspection carried out.","2020-01-19",null,"Completed","2020-01-17","No",null,null,"Internal"]
[null,null,null,null,null,"99_27/02/2020 08:29:57","2019-12-22","Defect","Ship Staff","Ship Staff Insp.","OWS bilge water inlet pipe leaking from various places and corroded.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related",10.29,"Medium","Not Applicable","Not Applicable","OWS bilge water inlet pipe removed, New pipe fabricated and put in place. ","2019-12-25",null,"Completed","2019-12-23","No",null,null,"Internal"]
[null,null,null,null,null,"99_27/02/2020 10:37:05","2019-12-30","Defect","Ship Staff","Ship Staff Insp.","Boiler # 1 flame eye found broken during trying out alarms.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Boiler # 1 Flame eye renewed with new spare.","2020-01-10",null,"Completed","2020-01-08","No",null,null,"Internal"]
[null,null,null,null,null,"99_27/02/2020 11:17:44","2020-01-26","Defect","Ship Staff","Ship Staff Insp.","AE # 1 unit # 4 & 5 cylinder head need to be inspected as the Pmax is low and Exh temp is high as compare to other units.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","AE # 3 & 4 Cylinder heads replaced with spare cylinder heads.","2020-01-30",null,"Completed","2020-01-29","No",null,null,"Internal"]
[null,null,null,null,null,"99_27/02/2020 11:26:09","2020-02-02","Defect","Ship Staff","Ship Staff Insp.","Air Ejector condenser drian sample chloride test carried out, Chloride value was overrange. ","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related",null,null,"Not Applicable","Not Applicable","Air Ejector condenser pressure tesated,LEaking tubes plugged. Condenser inlet side tubes found erroded from the ends. TO avoid further damage, Teflon tubes installed.","2020-03-02",null,"Completed","2020-02-04","No",null,null,"Internal"]
[null,null,null,null,null,"99_27/02/2020 11:34:16","2020-02-18","Breakdown","Ship Staff","Ship Staff Insp.","M.E unit # 3 exhaust temperature was very high and peak pressure was low.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","M.E unit # 3 Fuel injectors removed for inspeciton, found FWD side injector nozzle was broken. Spare injectores installed on both sides. ","2020-02-18",null,"Completed","2020-02-18","No",null,null,"Internal"]
[null,null,null,null,null,"99_27/02/2020 11:41:01","2020-02-15","Breakdown","Ship Staff","Ship Staff Insp.","Main Engine Unit # 4 No. 1 & 3 piston rings found broken during underpiston space inspection. ","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","M.E stopped, Unit # 4 piston removed and assembled with spare overhauled piston. Engine triedout, working satisfactorly.","2020-02-20",null,"Completed","2020-02-18","No",null,null,"Internal"]
[null,null,null,null,null,"99_27/02/2020 13:14:08","2020-02-15","Defect","Ship Staff","Ship Staff Insp.","AE # 2 Exhaust gas leaking from the  exhasut manifold connection to turbocharger.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","AE # 2 exhaust manifold connection removed, Gasket renewed. ","2020-02-24",null,"Completed","2020-02-20","No",null,null,"Internal"]
[null,null,null,null,null,"99_27/02/2020 13:20:11","2020-02-19","Breakdown","Ship Staff","Ship Staff Insp.","Main Air Compressor # 2, air leaking from last stage cooler cover.","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Main air compressor cooler cover removed, gasket renewed. Also during inspection it was observed that one of the cooler tube was leaking, same tube plugged. Comp. tried out, no leaks observed.","2020-02-25",null,"Completed","2020-02-21","No",null,null,"Internal"]
[null,null,null,null,null,"99_23/12/2019 8:12:07 PM","2019-12-11","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Engine room toilet door to be fitted back in place properly","Miscellaneous","Eng. / Strg. Comp.","Inappropriate Procedure",null,null,"Not Applicable","Not Applicable","Engine room toilet door hinge found broken. Hinge repaired. Door put back.","2020-03-11",null,"Completed","2020-01-18","No",null,null,"Internal"]
[null,null,null,null,null,"99_23/12/2019 8:21:38 PM","2019-12-11","Breakdown,Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Soft patch on FW generator SW out pipe","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related",10.3,"Medium","Not Applicable","Not Applicable","FWG new pipe fabricated and installed. No leaks observed.","2020-03-11",null,"Completed","2020-02-25","No",null,null,"Internal"]
[null,null,null,null,null,"99_23/12/2019 8:26:02 PM","2019-12-11","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Safety loop around ladder approximate 3.2 mtrs high going from ECR platform to top of ECR deck","Miscellaneous","Eng. / Strg. Comp.","Inappropriate Procedure",null,null,"Not Applicable","Not Applicable","Safety loop fabricated and installed.","2020-03-11",null,"Completed","2020-02-01","No",null,null,"Internal"]
[null,null,null,null,null,"99_23/12/2019 12:53:35 PM","2019-11-27","Defect","Ship Staff","Ship Staff Insp.","BALLAST, FUEL OIL, FRESH WATER TANK  VENT HEAD FLAME SCREENS FOUND WASTED & PAINTED","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related",11.7,"High","Not Applicable","Not Applicable","RENEWAL COMPLETED","2020-02-15",null,"Completed","2020-02-02","No",null,null,"Internal"]
[null,null,null,null,null,"99_23/12/2019 8:06:53 PM","2019-12-11","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Capacity for few drip trays missing","Deck - Pipe / Fittings","General Appearance","Inappropriate Procedure",null,null,"Not Applicable","Not Applicable","COMPLETED","2020-03-11",null,"Completed","2020-01-10","No",null,null,"Internal"]
[null,null,null,null,null,"99_24/12/2019 5:34:56 PM","2019-12-11","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Sight glass for port aft mooring winch having crack","Deck - Mooring Machinery","Mooring","Equipment Related",9.14,"Medium","Not Applicable","Not Applicable","Fabricated & Renewed","2020-02-15",null,"Completed","2020-02-08","No",null,null,"Internal"]
[null,null,null,null,null,"99_24/12/2019 12:07:14 PM","2019-12-11","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","GUIDE WIRE MISSING FOR PUMPROOM RESCUE ARRANGEMNET","Miscellaneous","General Appearance","Inappropriate Procedure",5.2,"Very High","Not Applicable","Not Applicable","GUIDE WIRE RIGGED","2020-01-30",null,"Completed","2019-12-30","No",null,null,"Internal"]
[null,null,null,null,null,"99_23/12/2019 10:35:30 PM","2019-11-27","Defect","Ship Staff","Ship Staff Insp.","SEVERAL VALVE WHEELS FOR DECK AIR LINE  FOUND BROKEN","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","Equipment Related",null,"Low","Not Applicable","Not Applicable"," RENEWED","2020-02-27",null,"Completed","2020-02-17","No",null,null,"Internal"]
[null,null,null,null,null,"99_23/12/2019 8:04:47 PM","2019-12-11","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Vent deflection plates holed on few vents like DB DO tank (s), FW tank, FW bosun store vent. Wire mesh also missing from few of them","Deck - Pipe / Fittings","General Appearance","Equipment Related",11.7,"High","Not Applicable","Not Applicable","TOTAL 41 VENT HEADS COVERS FABRICATED & FLAME SCREENS RENEWED","2020-03-11",null,"Completed","2020-01-29","No",null,null,"Internal"]
[null,null,null,null,null,"99_28/2/2020 1:47:46 PM","2020-01-20","Defect","Ship Staff","Ship Staff Insp."," Fire line section going to steering flat for sprinkler System for chemical locker found wasted & holed.","LSA / FFA","LSA / FFA Appliances","Equipment Related",11.4,"Very High","Not Applicable","Not Applicable","FABRICATED & RENEWED","2020-02-09",null,"Completed","2020-01-31","No",null,null,"Internal"]
[null,null,null,null,null,"99_28/2/2020 2:20:15 PM","2020-01-15","Defect","Ship Staff","Ship Staff Insp.","TOTAL 15 SECTIONS OF PNEUMATIC LINE ON MAIN DECK FOUND HEAVILY RUSTED & WASTED","Deck - Pipe / Fittings","General Appearance","Equipment Related",11.4,"Very High","Not Applicable","Not Applicable","FABRICATED & RENEWED","2020-03-30",null,"Completed","2020-02-20","No",null,null,"Internal"]
[null,null,null,null,null,"99_28/2/2020 2:25:47 PM","2020-02-08","Defect","Ship Staff","Ship Staff Insp.","3 SECTIONS OF FRESH WATER LINE ON MAIN DECK FOUND HEAVILY RUSTED & WASTED / HOLED","Deck - Pipe / Fittings,Miscellaneous","General Appearance","Equipment Related",11.4,"Very High","Not Applicable","Not Applicable","FABRICATED & RENEWED","2020-03-30",null,"Completed","2020-02-24","No",null,null,"Internal"]
[null,null,null,null,null,"99_28/2/2020 2:34:02 PM","2020-02-01","Defect","Ship Staff","Ship Staff Insp.","SIGHT GLASS OF DECK SEAL FOUND BROKEN","Inert Gas","Cargo / Ballast Systems","Equipment Related",8.27,"Medium","Not Applicable","Not Applicable","FABRICATED & RENEWED","2020-02-27",null,"Completed","2020-02-17","No",null,null,"Internal"]
[null,null,null,null,null,"99_28/2/2020 2:50:40 PM","2020-02-05","Defect","Ship Staff","Ship Staff Insp.","MF/HF & VHF ANTENNA SECURING BRACKETS FOUND WASTED & HOLED","Miscellaneous","General Appearance","Inappropriate Procedure",11.8,"Low","Not Applicable","Not Applicable","FABRICATED & RENEWED","2020-02-29",null,"Completed","2020-02-26","No",null,null,"Internal"]
[null,null,null,null,null,"99_28/2/2020 2:54:21 PM","2020-02-02","Defect","Ship Staff","Ship Staff Insp.","EMERGENCY GENERATOR OIL TANK VENT HEAD COVER FOUND WASTED & HOLED","Deck - Pipe / Fittings","General Appearance","Inappropriate Procedure",11.7,"High","Not Applicable","Not Applicable","FABRICATED & RENEWED","2020-02-10",null,"Completed","2020-02-04","No",null,null,"Internal"]
[null,null,null,null,null,"99_28/2/2020 3:14:24 PM","2020-02-02","Defect","Ship Staff","Ship Staff Insp."," No.7 foam monitor line found wasted & holed ","LSA / FFA","LSA / FFA Appliances","Equipment Related",11.4,"Very High","Not Applicable","Not Applicable","FABRICATED & RENEWED","2020-02-12",null,"Completed","2020-02-05","No",null,null,"Internal"]
[null,null,null,null,null,"99_21/3/2020 2:01:06 PM","2020-02-15","Defect","Ship Staff","Ship Staff Insp.","LUBE OIL / OILY BILGE PUMP EMEGENCY STOP BOX COVER  FOUND WASTED & HOLED","Miscellaneous","General Appearance","Equipment Related",null,null,"Not Applicable","Not Applicable","FABRICATED & RENEWED","2020-03-15",null,"Completed","2020-02-29","No",null,null,"Internal"]
[null,null,null,null,null,"99_24/12/2019 5:53:48 PM","2019-12-11","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","1 nos bottom step for outside ladder port side from bridge going to E-deck wasted and holed","Accommodation","Structural Condn. / WT integrity ","Inappropriate Procedure",11.8,"Low","Not Applicable","Not Applicable","FABRICATED & RENEWED","2020-12-30",null,"Completed","2020-02-27","Yes",null,null,"Internal"]
[null,null,null,null,null,"99_21/3/2020 2:09:34 PM","2020-02-28","Defect","Ship Staff","Ship Staff Insp.","WHEEL HOUSE NATURAL VENT HEAD COVER FOUND WASTED, HOLED & THINNED DOWN","Miscellaneous","Structural Condn. / WT integrity ","Inappropriate Procedure",11.2,"Medium","Not Applicable","Not Applicable","FABRICATED & RENEWED","2020-03-30",null,"Completed","2020-03-02","No",null,null,"Internal"]
[null,null,null,null,null,"99_21/3/2020 2:11:35 PM","2020-02-28","Defect","Ship Staff","Ship Staff Insp.","COP TRIP BOX OUTSIDE PUMPROOM FOUND WASTED, THINNED DOWN & HOLED","Miscellaneous","General Appearance","Inappropriate Procedure",null,null,"Not Applicable","Not Applicable","FABRICATED & RENEWED","2020-03-30",null,"Completed","2020-03-03","No",null,null,"Internal"]
[null,null,null,null,null,"99_21/3/2020 2:13:24 PM","2020-02-27","Defect","Ship Staff","Ship Staff Insp.","PROVISION CRANE STARTER BOX COVER FOUND WASTED & HOLED","Miscellaneous","General Appearance","Inappropriate Procedure",null,null,"Not Applicable","Not Applicable","FABRICATED & RENEWED","2020-03-30",null,"Completed","2020-03-04","No",null,null,"Internal"]
[null,null,null,null,null,"99_21/3/2020 2:15:44 PM","2020-03-06","Defect","Ship Staff","Ship Staff Insp.","DECK SEAL SIGHT GLASS & PLATE FOUND BROKEN & THINNED DOWN","Inert Gas","Cargo / Ballast Systems","Equipment Related",8.27,"Medium","Not Applicable","Not Applicable","RENEWED","2020-03-15",null,"Completed","2020-03-09","No",null,null,"Internal"]
[null,null,null,null,null,"99_21/3/2020 2:19:44 PM","2020-03-08","Defect","Ship Staff","Ship Staff Insp.","SEVEN FIRE & FOAM HYDRANTS ON DECK FOUND LEAKING","LSA / FFA","LSA / FFA Appliances","Equipment Related",5.35,"Medium","Not Applicable","Not Applicable","RENEWED","2020-03-25",null,"Completed","2020-03-12","No",null,null,"Internal"]
[null,null,null,null,null,"99_21/3/2020 2:28:18 PM","2020-03-15","Defect","Ship Staff","Ship Staff Insp.","FWD HYDRAULIC POWER PACK COOLER FOR MOORING PRESSURE GUAGE FOUND IN OPERATIONAL","Deck - Mooring Machinery","Mooring","Inappropriate Procedure",8.1300000000000008,"Medium","Not Applicable","Not Applicable","REHENWED","2020-03-25",null,"Completed","2020-03-16","No",null,null,"Internal"]
[null,null,null,null,null,"99_21/3/2020 2:53:54 PM","2020-03-14","Defect","Ship Staff","Ship Staff Insp.","DRAIN TO 4S COT VALVE FOUND LEAKING","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related",8.11,null,"Not Applicable","Not Applicable","SEAT RING RENEWED","2020-03-30",null,"Completed","2020-03-16","No",null,null,"Internal"]
[null,null,null,null,null,"99_21/3/2020 3:05:16 PM","2019-12-11","Defect","Ship Staff","Ship Staff Insp.","NO.1 & NO.3 STBD MANIFOLD MARPOL DRAIN VALVE LEAKING","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related",8.11,null,"Not Applicable","Not Applicable","SEAT RING RENEWED","2020-03-31",null,"Completed","2020-03-20","No",null,null,"Internal"]
[null,null,null,null,null,"99_23/3/2020 10:40:50 AM","2020-03-15","Defect","Ship Staff","Ship Staff Insp.","Both side MOB Lanyard found in old condition.","LSA / FFA","LSA / FFA Appliances","Equipment Related",null,null,"Not Applicable","Not Applicable","Need to Renew.","2020-03-15",null,"Completed","2020-03-15","No",null,null,"Internal"]
[null,null,null,null,null,"99_23/3/2020 2:06:37 PM","2020-01-20","Defect","Ship Staff","Ship Staff Insp.","M/E telegraph recorder not working, internal gears damaged","Navigation - Others","Navigation","Equipment Related",4.7,"High","Not Applicable","Not Applicable","New recorder unit recieved & replaced","2020-04-20","PERF200025","Completed","2020-03-15","No",null,null,"Internal"]
[null,null,null,null,null,"99_21/3/2020 3:27:55 PM","2020-03-17","Defect","Ship Staff","Ship Staff Insp.","NO.1 GEV Vave In AUS not opeartional remotely from CCR","Cargo Mach.","Cargo / Ballast Systems","Equipment Related",8.11,"Medium","Not Applicable","Not Applicable","RECTIFIED","2020-04-30",null,"Completed","2020-03-23","No",null,null,"Internal"]
[null,null,null,null,null,"99_22/3/2020 1:29:15 PM","2020-03-15","Defect","Ship Staff","Ship Staff Insp.","Steering gear natural vent not opening, Spindle moving freely, Need to open the vent cover & check the spindle & assembly.","Miscellaneous","Structural Condn. / WT integrity ","Inappropriate Procedure",11.7,"High","Not Applicable","Not Applicable","Fabricated & Overhauled","2020-04-30",null,"Completed","2020-03-23","No",null,null,"Internal"]
[null,null,null,null,null,"99_23/3/2020 10:47:41 AM","2020-03-15","Defect","Ship Staff","Ship Staff Insp.","Both side lifeboat front glass transparent view not clear","LSA / FFA","LSA / FFA Appliances","Equipment Related",5.27,"Medium","Not Applicable","Not Applicable","Renewed","2020-03-31",null,"Completed","2020-03-24","No",null,null,"Internal"]
[null,null,null,null,null,"99_24/12/2019 10:23:06 PM","2019-12-11","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Scavenge air receiver pressure gauge broken","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related",8.23,"Medium","Not Applicable","Not Applicable","Pressure gauge  renewed.","2020-03-11",null,"Completed","2020-02-12","No",null,null,"Internal"]
[null,null,null,null,null,"99_23/12/2019 8:23:45 PM","2019-12-11","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Tell Tale signs of leakage from No-2 Man engine jacket FW preheater end cover","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related",10.3,"Medium","Not Applicable","Not Applicable","Main engine jacket FW preheater bolts retightened. No leakages observed.","2020-03-11",null,"Completed","2020-02-16","No",null,null,"Internal"]
[null,null,null,null,null,"99_26/03/2020 03:21:17","2020-01-21","Defect","Ship Staff","Ship Staff Insp.","Engine room toilet door doesnt have locking arrangement from inside.","Miscellaneous","Eng. / Strg. Comp.","Inappropriate Procedure",10.3,"Medium","Not Applicable","Not Applicable","Engine room toilet door locking unit renewed.","2020-03-21",null,"Completed","2020-02-23","No",null,null,"Internal"]
[null,null,null,null,null,"99_26/03/2020 03:30:10","2020-02-25","Defect","Ship Staff","Ship Staff Insp.","Fire Hydrant near Purifier room leaking from the seat.","LSA / FFA","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Fire hydrant renewed.","2020-02-29",null,"Completed","2020-02-27","No",null,null,"Internal"]
[null,null,null,null,null,"99_26/03/2020 03:40:57","2020-02-24","Defect","Ship Staff","Ship Staff Insp.","M.E Unit # 3 crankcase door bottom latch not tightening completely, casuing Oil to leak.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related",10.3,"Medium","Not Applicable","Not Applicable","Door latch removed, FOund threads were damaged. All Outside and inside threads retapped. Latch put back, Tightening properly.","2020-03-02",null,"Completed","2020-02-29","No",null,null,"Internal"]
[null,null,null,null,null,"99_26/03/2020 03:44:50","2020-02-29","Breakdown","Ship Staff","Ship Staff Insp.","Emcy DG hydraulic starting hand pump not pumping above 200 bar and slips during pumping.","Critical Equip.","Emgcy. Systems","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Hyd pump plunger dismantled, Found O-ring inside was damaged causing oil to bypass. O-ring renewed, Plunger boxed back, Pump tried oout, working satisfactorly.","2020-03-02",null,"Completed","2020-03-01","No",null,null,"Internal"]
[null,null,null,null,null,"99_26/03/2020 03:50:12","2020-03-05","Breakdown","Ship Staff","Ship Staff Insp.","During cargo testing, boiler # 1 main feed water line started leaking from the middle of the pipe.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related",10.3,"Medium","Not Applicable","Not Applicable","Boiler feed water pipe removed, New pipe fabricated and put in place. No leaks observed.","2020-03-06",null,"Completed","2020-03-06","No",null,null,"Internal"]
[null,null,null,null,null,"99_26/03/2020 03:54:55","2020-03-05","Defect","Ship Staff","Ship Staff Insp.","Air ejector steam trap not operating properly as required.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related",10.3,"Medium","Not Applicable","Not Applicable","Air ejector steam trap opened up for inspection, found dirt inside, same cleaned and put back.","2020-03-10",null,"Completed","2020-03-08","No",null,null,"Internal"]
[null,null,null,null,null,"99_26/03/2020 03:59:30","2020-03-08","Defect","Ship Staff","Ship Staff Insp.","Sewage treatment plant scum flow not observed from the transparent pipe.","Critical Equip.","Eng. / Strg. Comp.","Equipment Related",10.31,"Very High","Not Applicable","Not Applicable","Scup flow pipe removed, Found sludge accumulated in teh pipe which was restricting the flow. Pipe cleared and put back. Scum flowing normally.","2020-03-10",null,"Completed","2020-03-09","No",null,null,"Internal"]
[null,null,null,null,null,"99_26/03/2020 04:05:31","2020-03-12","Defect","Ship Staff","Ship Staff Insp.","M.E unit # 6 fuel pump drain connection leaking from the washer.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Fuel pump drain connection removed, surface cleaned, washer renewed. Put back in use. No leaks observed.","2020-03-14",null,"Completed","2020-03-13","No",null,null,"Internal"]
[null,null,null,null,null,"99_26/03/2020 06:02:28","2020-03-11","Defect","Ship Staff","Ship Staff Insp.","M.E Unit # 4 piston ring# 1, 2 & 3 found broken from the but joints during under piston inspection. ","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","M.E unit # 4 Piston removed, replaced with spare new piston crown & skirt. Also Liner removed and replaced wiht old spare liner as the measurements were very high.","2020-03-20",null,"Completed","2020-03-16","No",null,null,"Internal"]
[null,null,null,null,null,"99_26/03/2020 06:07:48","2020-03-12","Defect","Ship Staff","Ship Staff Insp.","HFO purifier # 1 leaking from top cover during operation.","E/R - Purifier","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","HFO purifeir # 1 top cover removed, O-rings renewed, Purifier started, no leaks observed.","2020-03-20",null,"Completed","2020-03-17","No",null,null,"Internal"]
[null,null,null,null,null,"99_26/03/2020 06:11:16","2020-03-18","Defect","Ship Staff","Ship Staff Insp.","M.E unit # 4 fuel pump drain connection leaking from washer.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","M.E unit # 4 fuel pump drain connection removed, surface cleaned, washer renewed. Connection put back, no lekas observed.","2020-03-20",null,"Completed","2020-03-20","No",null,null,"Internal"]
[null,null,null,null,null,"99_26/03/2020 06:16:31","2020-03-20","Defect","Ship Staff","Ship Staff Insp.","Galley water overboard pipe chocked as galley water not draining.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related",10.3,"Medium","Not Applicable","Not Applicable","Galley water overboard pipe bottom section removed, found sludge deposit on the valve seat. same cleared. Pipe put back. One section pipe was having a  pin hole. same welded. ","2020-03-21",null,"Completed","2020-03-21","No",null,null,"Internal"]
[null,null,null,null,null,"99_26/03/2020 06:19:16","2019-03-15","Defect","Ship Staff","Ship Staff Insp.","M.E unit # 2 fwd fuel oil HP pipe leaking from fuel pump side connection.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","M.E unit # 2 pipe removed, Both side surface cleaned, distance checked, Pipe put back, no leaks observed.","2020-03-25",null,"Completed","2020-03-22","No",null,null,"Internal"]
[null,null,null,null,null,"99_26/03/2020 06:25:20","2020-03-15","Defect","Ship Staff","Ship Staff Insp.","HFO transfer pump slight leaking from the seal and creating some abnormal sound during running.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","HFO transfer pump dismantled for inspection, found stationary part of seal damaged, On further inspecton it was observed that bush bearing soft metal squeezed out. Othe side cover also removed and the beraing were found in bad condition. ALl 4 bush bearings, Mechanical seal & shaft seal renewed. Pump tried out, no abnormal sound or leakage observed.","2020-03-30",null,"Completed","2020-03-24","No",null,null,"Internal"]
[null,null,null,null,null,"99_26/03/2020 08:22:08","2020-03-10","Defect","Ship Staff","Ship Staff Insp.","AE Fuel Oil Autobackwash bypass filter leaking from flange connections.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related",10.3,"Medium","Not Applicable","Not Applicable","AE F.O autobackwash bypass filter connections removed, surface cleaned and new gasket installed. No leaks observed.","2020-03-30",null,"Completed","2020-03-24","No",null,null,"Internal"]
[null,null,null,null,null,"99_26/03/2020 08:26:08","2020-03-24","Defect","Ship Staff","Ship Staff Insp.","Deck air compressor not building up pressure.","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Deck air compressor cover removed, found the belts were not in good condition, all 3 belts renewed. Also L.O filters renewed. COmpressor tried out, working satisfactorly.","2020-03-25",null,"Completed","2020-03-24","No",null,null,"Internal"]
[null,null,null,null,null,"99_26/03/2020 09:30:20","2020-03-24","Defect","Ship Staff","Ship Staff Insp.","M.E unit # 1 FWD FUEL INJECTOR LEAKING FROM THE NUT.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","M.E UNIT # 1 BOTH FUEL INJECTORS REMOVED AS THE RUNNING HOURS WERE 6500 Hrs. BOTH REPLACED WITH OVERHAULED SPARE INJECTORES WITH NEW SPINDLE GUIDE AND NON RETURN VALVE.","2020-03-25",null,"Completed","2020-03-25","No",null,null,"Internal"]
[null,null,null,null,null,"99_26/03/2020 09:33:51","2020-03-15","Defect","Ship Staff","Ship Staff Insp.","M.E unit # 3 & 4 oil leaking from Crankcase doors.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","M.E unit # 3 & 4 crankcase doors old O-rings removed, surface cleaned, New O-rings installed. No leaks observed.","2020-03-30",null,"Completed","2020-03-25","No",null,null,"Internal"]
[null,null,null,null,null,"99_26/03/2020 09:38:46","2020-03-25","Breakdown","Ship Staff","Ship Staff Insp.","During M.E Crankcase inspection unit# 4 stuffing box drain pipe found broken from the welding joints.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","M.E stuffing box pipe removed, new pipe fabricated with one single length of pipe (no joints in between). Pipe put back. clamps adjusted and tightened properly. M.E turned, no contact observed.","2020-03-25",null,"Completed","2020-03-25","No",null,null,"Internal"]
[null,null,null,null,null,"99_26/03/2020 09:43:52","2020-03-15","Defect","Ship Staff","Ship Staff Insp.","Various places steam leaking from valve bonnets and flanges. Need to attend all leaks during anchorage.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related",10.3,"Medium","Not Applicable","Not Applicable","Various places steam leaks rectified. Bonnet and flange gaskets renewed. One valve bonnet bolts found broken, same drilled and retapped. laggings renewed where ever damaged.","2020-03-30",null,"Completed","2020-03-26","No",null,null,"Internal"]
[null,null,null,null,null,"99_25/3/2020 12:48:33 PM","2020-03-24","Defect","Ship Staff","Ship Staff Insp.","Port side windlass hydraulic line pressure side connecting to control lever found wasted & thinned down from bend","Deck - Mooring Machinery","Mooring","Equipment Related",11.4,"Very High","Not Applicable","Not Applicable","fabricated & renewed","2020-04-30",null,"Completed","2020-03-27","No",null,null,"Internal"]
[null,null,null,null,null,"99_21/3/2020 3:18:57 PM","2020-03-06","Defect","Ship Staff","Ship Staff Insp.","Stbd Provision Crane Operating platform railing damaged & wasted","Deck - Machinery,Miscellaneous","General Appearance","Inappropriate Procedure",null,null,"Not Applicable","Not Applicable","Fabricated & renewed","2020-04-30",null,"Completed","2020-03-30","No",null,null,"Internal"]
[null,null,null,null,null,"99_22/3/2020 1:22:50 PM","2020-03-12","Defect","Ship Staff","Ship Staff Insp.","Fixed gas detection system for ballast tank & spaces after running for few hours gives detector/ sensor fault","Miscellaneous","Cargo / Ballast Systems","Equipment Related",null,null,"Not Applicable","Not Applicable","RECTIFIED","2020-04-30",null,"Completed","2020-04-04","No",null,null,"Internal"]
[null,null,null,null,null,"99_7/4/2020 11:34:25 PM","2020-04-04","Defect","Ship Staff","Ship Staff Insp.","One section of Pneumatic line on deck found wasted & holed","Deck - Pipe / Fittings","General Appearance","Equipment Related",11.4,"Very High","Not Applicable","Not Applicable","Fabricated & Renwed","2020-04-30",null,"Completed","2020-04-05","No",null,null,"Internal"]
[null,null,null,null,null,"99_7/4/2020 11:37:53 PM","2020-03-28","Defect","Ship Staff","Ship Staff Insp."," 3 sections of fresh water line on main deck found wasted & holed","Deck - Pipe / Fittings","General Appearance","Equipment Related",11.4,"Very High","Not Applicable","Not Applicable","Fabricated & Renewed","2020-04-30",null,"Completed","2020-04-07","No",null,null,"Internal"]
[null,null,null,null,null,"99_10/4/2020 6:33:52 PM","2020-04-05","Defect","Ship Staff","Ship Staff Insp.","One sections of Pneumatic line on Main deck found holed & wasted","Deck - Pipe / Fittings","General Appearance","Equipment Related",11.4,"Very High","Not Applicable","Not Applicable","Fabricated & Rnewed","2020-04-15",null,"Completed","2020-04-08","No",null,null,"Internal"]
[null,null,null,null,null,"99_10/4/2020 6:35:52 PM","2020-04-04","Defect","Ship Staff","Ship Staff Insp."," 3 Section of Fresh water line on main deck found holed","Deck - Pipe / Fittings","General Appearance","Equipment Related",11.4,"Very High","Not Applicable","Not Applicable","Fabricated & Renewed","2020-04-30",null,"Completed","2020-04-10","No",null,null,"Internal"]
[null,null,null,null,null,"99_10/4/2020 6:38:32 PM","2020-04-02","Defect","Ship Staff","Ship Staff Insp.","Valve hydraulic steel tubing found leaking at Focsle & NEAR 2C COT","Deck - Pipe / Fittings","General Appearance","Equipment Related",11.4,"Very High","Not Applicable","Not Applicable","Steel tubing & Armato coulping renewed","2020-04-30",null,"Completed","2020-04-09","No",null,null,"Internal"]
[null,null,null,null,null,"99_23/3/2020 10:33:19 AM","2019-12-15","Defect","Ship Staff","Ship Staff Insp.","Fwd Life Jacket Box Cover near fwd Life raft found wasted & holed.","LSA / FFA","LSA / FFA Appliances","Equipment Related",null,null,"Not Applicable","Not Applicable","Fabricated & renewed","2020-04-15",null,"Completed","2020-04-09","No",null,null,"Internal"]
[null,null,null,null,null,"99_13/4/2020 7:40:45 PM","2020-03-23","Defect","Ship Staff","Ship Staff Insp.","Hydraulic leak found on port hose handling crane wire winch block","Deck - Machinery","General Appearance","Equipment Related",8.5,"Medium","Not Applicable","Not Applicable","Oring renewed","2020-05-30",null,"Completed","2020-04-11","No",null,null,"Internal"]
[null,null,null,null,null,"99_14/4/2020 6:46:53 PM","2020-04-01","Defect","Ship Staff","Ship Staff Insp.","One section of Valve hydraulic steel tubing found wasted & leaking","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related",11.4,"Very High","Not Applicable","Not Applicable","Renewed","2020-04-30",null,"Completed","2020-04-11","No",null,null,"Internal"]
[null,null,null,null,null,"99_14/4/2020 7:20:31 PM","2020-04-02","Defect","Ship Staff","Ship Staff Insp.","Several mooring winches Brake band elbows & pin found frozen Because of paint","Deck - Mooring Machinery","Mooring","Equipment Related",9.14,"Medium","Not Applicable","Not Applicable","Opened / Freed & greased","2020-05-15",null,"Completed","2020-04-14","No",null,null,"Internal"]
[null,null,null,null,null,"99_14/4/2020 7:22:56 PM","2020-04-06","Defect","Ship Staff","Ship Staff Insp.","APK Sounding pipe found broken & wasted","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related",null,null,"Not Applicable","Not Applicable","Fabricated & renewed","2020-05-30",null,"Completed","2020-04-11","No",null,null,"Internal"]
[null,null,null,null,null,"99_23/3/2020 10:10:52 AM","2020-03-05","Defect","Ship Staff","Ship Staff Insp.","Immersion Suit could not hold air pressure during test.","LSA / FFA","LSA / FFA Appliances","Equipment Related",5.33,"High","Not Applicable","Not Applicable","Received 4 pcs of Immersion suit on 02 april 2020 at singapore.","2020-03-31",null,"Completed","2020-04-02","No",null,null,"Internal"]
[null,null,null,null,null,"99_15/4/2020 8:24:39 PM","2020-04-04","Defect","Ship Staff","Ship Staff Insp.","SIX Mooring winch operating  lever guide / cover found wasted & holed","Deck - Mooring Machinery","Mooring","Equipment Related",null,null,"Not Applicable","Not Applicable","Fabricated & renewed","2020-05-30",null,"Completed","2020-04-15","No",null,null,"Internal"]
[null,null,null,null,null,"99_15/4/2020 8:40:02 PM","2020-04-06","Defect","Ship Staff","Ship Staff Insp.","Mast riser flame screen found holed","Inert Gas","Cargo / Ballast Systems","Equipment Related",8.19,"High","Not Applicable","Not Applicable","Renewed","2020-04-15",null,"Completed","2020-04-10","No",null,null,"Internal"]
[null,null,null,null,null,"99_16/4/2020 3:39:44 PM","2020-04-02","Defect","Ship Staff","Ship Staff Insp.","Port side hose handling crane Jib pin/ Hinge was frozen. Because of that Noise was coming while lowering & heaving the Jib","Deck - Machinery","Cargo / Ballast Systems","Equipment Related",8.5,"Medium","Not Applicable","Not Applicable","Lubricated & greased.","2020-04-30",null,"Completed","2020-04-11","No",null,null,"Internal"]
[null,null,null,null,null,"99_16/4/2020 3:45:57 PM","2020-04-06","Defect","Ship Staff","Ship Staff Insp.","Both gangway wire sheaves found dry.","Deck - Machinery","General Appearance","Equipment Related",5.47,"Medium","Not Applicable","Not Applicable","Lubricated & greased","2020-05-15",null,"Completed","2020-04-16","No",null,null,"Internal"]
[null,null,null,null,null,"99_16/4/2020 8:39:53 PM","2020-04-06","Defect","Ship Staff","Ship Staff Insp.","Pressure guage box cover for tank cleaning heater outside pumproom found wasted & holed","Miscellaneous","General Appearance","Equipment Related",null,null,"Not Applicable","Not Applicable","Fabricated & Renewed","2020-05-15",null,"Completed","2020-04-16","No",null,null,"Internal"]
[null,null,null,null,null,"99_15/4/2020 8:28:45 PM","2020-02-15","Defect","Ship Staff","Ship Staff Insp.","Several valve wheels of steam line, fresh water line, pneumatic line on main deck found broken","Deck - Pipe / Fittings","General Appearance","Equipment Related",null,null,"Not Applicable","Not Applicable","Renewal completed","2020-04-30",null,"Completed","2020-04-16","No",null,null,"Internal"]
[null,null,null,null,null,"99_16/4/2020 8:57:18 PM","2020-04-10","Defect","Ship Staff","Ship Staff Insp.","Deck seal sight glass found cracked","Inert Gas","Cargo / Ballast Systems","Equipment Related",8.27,"Medium","Not Applicable","Not Applicable","Renewed","2020-04-30",null,"Completed","2020-04-17","No",null,null,"Internal"]
[null,null,null,null,null,"99_17/4/2020 1:04:40 PM","2020-04-04","Defect","Ship Staff","Ship Staff Insp.","Port side Ramp / Step for standing during anchor station fwd found wasted.","Miscellaneous","General Appearance","Equipment Related",null,null,"Not Applicable","Not Applicable","Fabricated ","2020-04-30",null,"Completed","2020-04-10","No",null,null,"Internal"]
[null,null,null,null,null,"99_17/4/2020 1:06:36 PM","2020-04-06","Defect","Ship Staff","Ship Staff Insp.","Stbd gangway wire protection cover found wasted & holed","Miscellaneous","General Appearance","Equipment Related",null,null,"Not Applicable","Not Applicable","Fabricated & renewed","2020-05-15",null,"Completed","2020-04-18","No",null,null,"Internal"]
[null,null,null,null,null,"99_18/4/2020 9:10:13 PM","2020-04-01","Defect","Ship Staff","Ship Staff Insp.","Port side crane operating lever found wasted ","Miscellaneous","General Appearance","Equipment Related",null,null,"Not Applicable","Not Applicable","Fabricated & renewed","2020-05-30",null,"Completed","2020-04-18","No",null,null,"Internal"]
[null,null,null,null,null,"99_18/4/2020 9:17:26 PM","2020-03-09","Observation","Owner / Marine / Tech. Suptd.","ISM Audit","12.20.05.011.04 - Pre arrival and commencement of cargo operation checklist for loading at Jose Sec B (24 Hrs Prior Operation) completed on 15 Jan at 1045 Hrs, however Operations commenced on 18 Jan 2019.\r\nSection B to be reviewed and re-signed in case cargo operations is delayed.\r\n","Documentation","ISM Related","Inappropriate Procedure",null,null,"Not Applicable","Not Applicable","Section B reveiwed again within 24 hrs of starting of opeartion","2020-04-30",null,"Completed","2020-04-10","No",null,null,"Internal"]
[null,null,null,null,null,"99_18/4/2020 9:20:10 PM","2020-03-09","Observation","Owner / Marine / Tech. Suptd.","ISM Audit","12.20.05.011.04 - Pre arrival and commencement of cargo operation checklist for loading at Jose Sec D (Prior start of Operation) completed on 16 Jan at 1048 Hrs, however Operations commenced on 18 Jan 2019 0200 hrs.\r\nSection D to be completed just prior the commencement of operation.\r\n","Documentation","ISM Related","Human Error,Inappropriate Procedure",null,null,"Not Applicable","Not Applicable","Reviewed again prior start of operation","2020-04-30",null,"Completed","2020-04-10","No",null,null,"Internal"]
[null,null,null,null,null,"99_17/4/2020 7:56:44 PM","2020-04-17","Defect","Ship Staff","Ship Staff Insp.","No.1 Red manifold drain valve ( Stripper Discharge ) Port side suspect leaking","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related",8.11,"Medium","Not Applicable","Not Applicable","Seatring Renewed","2020-05-15",null,"Completed","2020-04-19","No",null,null,"Internal"]
[null,null,null,null,null,"99_24/4/2020 7:01:47 PM","2020-04-22","Defect","Ship Staff","Ship Staff Insp.","Air line on deck going to stbd gangway found holed","Deck - Pipe / Fittings","General Appearance","Equipment Related",11.4,"Very High","Not Applicable","Not Applicable","Fabricated & renewed","2020-04-26",null,"Completed","2020-04-24","No",null,null,"Internal"]
[null,null,null,null,null,"99_30/04/2020 16:56:07","2020-03-28","Defect","Ship Staff","Ship Staff Insp.","M.E F.O AUTOBACKWASH FILTER LEAKING FROM TOP COVER.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related",10.3,"High","Not Applicable","Not Applicable","M.E F.O AUTOBACK WASH FILTER TOP COVER REMOVED, FOUND SEAL RINGS DAMAGED, SAME RENEWED. TOP COVER PUT BACK, NO LEAKS OBSERVED.","2020-04-05",null,"Completed","2020-04-01","No",null,null,"Internal"]
[null,null,null,null,null,"99_30/04/2020 17:01:20","2020-03-15","Defect","Ship Staff","Ship Staff Insp.","FWG JCFW INLET VALVE LEAKING DUE TO WHICH, FWG EVAPORATOR CANNOT BE OPENED UP FOR MANUAL CLEANING.\t","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related",10.3,"Medium","Not Applicable","Not Applicable","M.E JACKET COOLING SYSTEM ISOLATED, FWG JCFW VALVE REMOVED AND REPLACED WITH NEW SPARE VALVE. ","2020-05-15",null,"Completed","2020-04-03","No",null,null,"Internal"]
[null,null,null,null,null,"99_30/04/2020 17:05:44","2020-04-10","Defect","Ship Staff","Ship Staff Insp.","FWG EJECTOR PUMP DISCHARGE VALVE LEAKING FROM BODY DUE TO PIN HOLE.\t","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related",10.3,"High","Not Applicable","Not Applicable","FWG EJECTOR PUMP DISCHARGE VALVE REMOVED AND RELACED WITH NEW SPARE VALVE. NO LEAKS OBSERVED.","2020-05-10",null,"Completed","2020-04-17","No",null,null,"Internal"]
[null,null,null,null,null,"99_30/04/2020 17:09:54","2020-04-12","Defect","Ship Staff","Ship Staff Insp.","M.E TURBOCHARGER # 1 GRID WASHING LINE CHOKE.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related",10.34,"High","Not Applicable","Not Applicable","M.E TURBOCHARGER # 1 GRID WASHING LINE & CONTAINER REMOVED AND CLEARED.","2020-04-19",null,"Completed","2020-04-19","No",null,null,"Internal"]
[null,null,null,null,null,"99_23-12-2019 13:09:00","2019-12-11","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","No-1 main C.S.W pump mechanical seal leaking","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related",10.3,"Medium","Not Applicable","Not Applicable","PUMP OPENED UP FOR INSPECTION, FOUND MECHANICAL SEAL SPRING BROKEN, SEAL SPRING REPLACED WITH OLD SPARE SPRING (NO NEW SEAL ONBOARD). PUMP BOXED BACK AND TRIED OUT, NO LEAKS OBSERVED","2020-03-11","PERF200005","Completed","2020-04-20","No",null,null,"Internal"]
[null,null,null,null,null,"99_30/04/2020 17:46:11","2020-03-26","Defect","Ship Staff","Ship Staff Insp.","FWG EJECTOR PUMP NOT BUILDING UP ENOUGH PRESSURE FOR MAINTAIN REQUIRED VACUUM.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related",10.3,"Medium","Not Applicable","Not Applicable","Ejector pump opened up for inspection, Found impeller locking bolts missing and washer stuck in the pump housing. Bottom wear ring completely wasted (No wear ring), Impeller removed, found bottom wear ring broken parts stuck inside and top impeller mouth ring was damaged. Mechanical seal removed, found rotating part broken. Shaft found cracked from the key way same welded and machined. Bottom wear ring housing gringed to make surface parallel. New wear ring installed and locked with grub screw. Pump body assembled with old spare impeller. Pump boxed back, pump tried out slight improvement in the pressure.","2020-04-26",null,"Completed","2020-04-07","No",null,null,"Internal"]
[null,null,null,null,null,"99_30/04/2020 18:00:09","2020-04-06","Defect","Ship Staff","Ship Staff Insp.","M.E Fuel oil Supply pump # 2 leaking from seal.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related",10.3,"High","Not Applicable","Not Applicable","M.E F.O supply pump # 2 opened up for inspection. All parts cleaned and inspected, found slight damage on seal. Mechanical seal and oil seal renewed, also both sides gaskets renewed. Pump boxed back and triedout, no leaks observed.","2020-05-06",null,"Completed","2020-04-23","No",null,null,"Internal"]
[null,null,null,null,null,"99_30/04/2020 18:08:25","2020-03-17","Defect","Ship Staff","Ship Staff Insp.","Engine room 3rd deck STBD side drain lines chocked.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related",10.3,"Medium","Not Applicable","Not Applicable","Engine room 3rd deck Drain lines removed, Lines cleared and put back.","2020-05-17",null,"Completed","2020-04-27","No",null,null,"Internal"]
[null,null,null,null,null,"99_21/12/2019 5:20:37 PM","2019-12-19","Breakdown","Ship Staff","Ship Staff Insp.","AE # 1 CENTRIFUGAL FILTER PUMPS MOTOR WINDING DAMAGED.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related",null,null,"Not Applicable","Not Applicable","AE # 1 CENTRIFUGAL FILTER PUMPS MOTOR RENEWED.","2020-03-19","0097-2019","Completed","2020-04-05","No",null,null,"Internal"]
[null,null,null,null,null,"99_27/3/2020 12:51:18 AM","2020-02-01","Defect","Ship Staff","Ship Staff Insp.","PA system speaker on monkey island inoperational","Navigation - Others","Navigation","Equipment Related",4.7,"High","Not Applicable","Not Applicable","Spare recieved, renewed","2020-05-01","PERF200029","Completed","2020-04-10","No",null,null,"Internal"]
[null,null,null,null,null,"99_27/3/2020 12:55:43 AM","2020-03-15","Defect","Ship Staff","Ship Staff Insp.","Stbd side ECDIS mouse, zoom in zoom out wheel not working ","Navigation - ECDIS","Navigation","Equipment Related",4.7,"High","Not Applicable","Not Applicable","Mouse recieved from Wartsila & renewed.","2020-04-15","SR200024","Completed","2020-04-04","No",null,null,"Internal"]
[null,null,null,null,null,"99_27/3/2020 1:02:02 AM","2020-02-01","Defect","Ship Staff","Ship Staff Insp.","ECDIS showing update failed in ‘update log’ if updated by normal weekly procedure – Vsl currently deletes & reinstalls all ENC’s weekly ","Navigation - ECDIS","Navigation","Equipment Related",4.7,"High","Not Applicable","Not Applicable","patch file installed by technician, no error seen","2020-05-01",null,"Completed","2020-03-28","No",null,null,"Internal"]
[null,null,null,null,null,"99_30/4/2020 6:59:43 PM","2020-04-15","Defect","Ship Staff","Ship Staff Insp.","4 section of Fresh water line on main dck found wasted & heavily rusted","Deck - Pipe / Fittings","General Appearance","Equipment Related",11.4,"Very High","Not Applicable","Not Applicable","Fabricated & renewed","2020-04-30",null,"Completed","2020-04-28","No",null,null,"Internal"]
[null,null,null,null,null,"99_30/4/2020 7:02:13 PM","2020-04-15","Defect","Ship Staff","Ship Staff Insp.","10 Pcs winch lever guide cover found wasted & holed of Fwd winches","Deck - Mooring Machinery","Mooring","Equipment Related",null,null,"Not Applicable","Not Applicable","Fabricated & renewed","2020-05-30",null,"Completed","2020-04-27","No",null,null,"Internal"]
[null,null,null,null,null,"99_30/4/2020 7:06:50 PM","2020-04-15","Defect","Ship Staff","Ship Staff Insp.","Three sections of Fresh water line on main deck found wasted & heavily rusted","Deck - Pipe / Fittings","General Appearance","Equipment Related",11.4,"Very High","Not Applicable","Not Applicable","Fabricated & renewed","2020-05-15",null,"Completed","2020-04-30","No",null,null,"Internal"]
[null,null,null,null,null,"99_7/4/2020 11:30:17 PM","2020-04-02","Defect","Ship Staff","Ship Staff Insp.","Yellow line drop valve on main deck  leaking, suspect seat ring damaged","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related",8.11,"Medium","Not Applicable","Not Applicable","Seatring Renewed","2020-04-30",null,"Completed","2020-04-30","No",null,null,"Internal"]
[null,null,null,null,null,"99_23/3/2020 10:07:01 AM","2020-03-07","Defect","Ship Staff","Ship Staff Insp.","No 7 foam Monitor having small leak.","LSA / FFA","LSA / FFA Appliances","Equipment Related",11.7,"High","Not Applicable","Not Applicable","Valve Renewed","2020-05-15",null,"Completed","2020-05-01","No",null,null,"Internal"]
[null,null,null,null,null,"99_15/4/2020 3:15:56 PM","2020-04-10","Other","Ship Staff","Ship Staff Insp.","Both side life boat davits rusted.","LSA / FFA","LSA / FFA Appliances","External Factors",null,null,"Not Applicable","Not Applicable","Derusting & Painting completed","2020-06-10",null,"Completed","2020-05-06","No",null,null,"Internal"]
[null,null,null,null,null,"99_23-12-2019 13:11:56","2019-12-11","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Tell-tale signs of leakage from No-2 main C.S.W pump discharge valve sacificial flange","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related",10.3,"Medium","Not Applicable","Not Applicable","MCSW pump flange connection bolts tightened as were loose. No leaks observed.","2020-03-11","PERF200060","Completed","2020-02-06","No",null,null,"Internal"]
[null,null,null,null,null,"99_15/5/2020 8:30:05 AM","2020-04-11","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Electrical panels in purifier room are very dirty. To be cleaned ","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related",10.3,"High","Not Applicable","Not Applicable","Electrical panel in purifier room cleaned.","2020-05-11",null,"Completed","2020-04-20","No",null,null,"Internal"]
[null,null,null,null,null,"99_15/5/2020 8:32:17 AM","2020-04-11","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ME Foundation bolts to be greased. ","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related",10.3,"Medium","Not Applicable","Not Applicable","M.E foundation bolts threads cleaned and greased. ","2020-05-11",null,"Completed","2020-05-03","No",null,null,"Internal"]
[null,null,null,null,null,"99_15/5/2020 8:36:13 AM","2020-04-11","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","E/R Bilges painting to be completed. ","Miscellaneous","Eng. / Strg. Comp.","Inappropriate Procedure",10.3,"Medium","Not Applicable","Not Applicable","E/R bilges cleaning and painting carried out.","2020-05-11",null,"Completed","2020-05-02","No",null,null,"Internal"]
[null,null,null,null,null,"99_15/05/2020 10:06:18","2020-04-11","Defect","Ship Staff","Suptd. Insp.","Engine room casing some of the lights are in fused condition. Same to be renewed. ","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related",null,null,"Not Applicable","Not Applicable","Fused lights renewed.","2020-04-26",null,"Completed","2020-04-15","No",null,null,"Internal"]
[null,null,null,null,null,"99_21/3/2020 3:09:31 PM","2020-03-17","Defect","Ship Staff","Ship Staff Insp.","NO.1 Stbd Manifold valve Suspect leaking","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related",8.11,"Medium","Not Applicable","Not Applicable","Checked during pressure testing & discharging opeartion, No leaks found","2020-06-29",null,"Completed","2020-05-16","No",null,null,"Internal"]
[null,null,null,null,null,"99_17/4/2020 1:21:45 PM","2020-04-06","Defect","Ship Staff","Ship Staff Insp.","Mast riser platform on top closing arrangement cover not available","Miscellaneous","General Appearance","Equipment Related",null,null,"Not Applicable","Not Applicable","Fabricated & renewed","2020-06-15",null,"Completed","2020-05-07","No",null,null,"Internal"]
[null,null,null,null,null,"99_17/5/2020 12:23:39 PM","2020-04-11","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp."," Slop tank heating coils are in poor condition. To be de rusted and painted.","Deck - Pipe / Fittings","General Appearance","Equipment Related",8.15,"High","Not Applicable","Not Applicable","Derusted & painted","2020-07-15",null,"Completed","2020-04-15","No",null,null,"Internal"]
[null,null,null,null,null,"99_18/5/2020 12:58:23 PM","2020-04-15","Defect","Ship Staff","Ship Staff Insp.","3 Section of Fresh water line found wasted & holed","Deck - Pipe / Fittings","General Appearance","Equipment Related",11.4,"Very High","Not Applicable","Not Applicable","Fabricated & renewed","2020-06-15",null,"Completed","2020-05-01","No",null,null,"Internal"]
[null,null,null,null,null,"99_18/5/2020 1:04:20 PM","2020-04-23","Defect","Ship Staff","Ship Staff Insp.","foam monitor Valve on deck found leaking","LSA / FFA","LSA / FFA Appliances","Equipment Related",5.35,"Medium","Not Applicable","Not Applicable","Valve renewed","2020-05-30",null,"Completed","2020-05-01","No",null,null,"Internal"]
[null,null,null,null,null,"99_18/5/2020 1:06:39 PM","2020-04-28","Defect","Ship Staff","Ship Staff Insp.","2 section of Pneumatic line on main deck found holed","Deck - Pipe / Fittings","General Appearance","Equipment Related",11.4,"Very High","Not Applicable","Not Applicable","Fabricated & renewed","2020-05-15",null,"Completed","2020-05-03","No",null,null,"Internal"]
[null,null,null,null,null,"99_18/5/2020 1:08:22 PM","2020-04-18","Defect","Ship Staff","Ship Staff Insp.","Foam breanch line on main deck found holed","LSA / FFA","LSA / FFA Appliances","Equipment Related",11.4,"Very High","Not Applicable","Not Applicable","Fabricated","2020-05-15",null,"Completed","2020-05-04","No",null,null,"Internal"]
[null,null,null,null,null,"99_18/5/2020 1:12:14 PM","2020-05-01","Defect","Ship Staff","Ship Staff Insp.","Seawater cooler line for aft winches found holed","Deck - Mooring Machinery","Mooring","Equipment Related",11.4,"Very High","Not Applicable","Not Applicable","Fabricated & renewed","2020-05-15",null,"Completed","2020-05-06","No",null,null,"Internal"]
[null,null,null,null,null,"99_18/5/2020 1:17:42 PM","2020-05-08","Defect","Ship Staff","Ship Staff Insp.","Seawater line valve going to foam pump in fire station for foam system found leaking","LSA / FFA","LSA / FFA Appliances","Equipment Related",5.38,"High","Not Applicable","Not Applicable","Same renewed","2020-05-30",null,"Completed","2020-05-13","No",null,null,"Internal"]
[null,null,null,null,null,"99_18/5/2020 1:19:41 PM","2020-05-11","Defect","Ship Staff","Ship Staff Insp.","Branch line to fire line on poop deck found holed & rusted","Deck - Pipe / Fittings","LSA / FFA Appliances","Equipment Related",11.4,"Very High","Not Applicable","Not Applicable","Fabricated & renewed","2020-05-30",null,"Completed","2020-05-14","No",null,null,"Internal"]
[null,null,null,null,null,"99_18/5/2020 1:21:32 PM","2020-05-08","Defect","Ship Staff","Ship Staff Insp.","1C COT Submerged cow machine valve found leaking during pressure testing","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related",8.11,null,"Not Applicable","Not Applicable","Valve renewed","2020-05-15",null,"Completed","2020-05-08","No",null,null,"Internal"]
[null,null,null,null,null,"99_18/5/2020 1:24:12 PM","2020-05-08","Defect","Ship Staff","Ship Staff Insp.","No.1 Red line drop valve found leaking/ pasing during pressure testing.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related",8.11,null,"Not Applicable","Not Applicable","Valve renewed","2020-05-15",null,"Completed","2020-05-10","No",null,null,"Internal"]
[null,null,null,null,null,"99_17/5/2020 12:33:47 PM","2020-04-11","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","All dressor couplings greasing to carry out and bolts to renew where required.","Deck - Pipe / Fittings","General Appearance","Equipment Related",11.5,"Medium","Not Applicable","Not Applicable","Greasing completed ","2020-06-15",null,"Completed","2020-05-03","No",null,null,"Internal"]
[null,null,null,null,null,"99_17/5/2020 12:47:21 PM","2020-04-11","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Provision room door lock handles to be renewed.","Miscellaneous","General Appearance","Equipment Related",null,null,"Not Applicable","Not Applicable","Fabricated & renewed","2020-06-15",null,"Completed","2020-04-14","No",null,null,"Internal"]
[null,null,null,null,null,"99_17/4/2020 9:06:53 PM","2020-04-03","Defect","Ship Staff","Ship Staff Insp.","No.1 & 3 COP Pneumatic discharge valve not closing remotely from CCR.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related",8.11,"Medium","Not Applicable","Not Applicable","Troubleshooting carried out, Both valves working from ccr","2020-06-30",null,"Completed","2020-05-22","No",null,null,"Internal"]
[null,null,null,null,null,"99_18/5/2020 1:43:04 PM","2020-05-20","Defect","Ship Staff","Ship Staff Insp.","Six section of Fresh water line on main deck found heavily rusted & wasted","Deck - Pipe / Fittings","General Appearance","Equipment Related",11.4,"Very High","Not Applicable","Not Applicable","Fabricated & renewed","2020-05-30",null,"Completed","2020-05-24","No",null,null,"Internal"]
[null,null,null,null,null,"99_17/5/2020 12:25:21 PM","2020-04-11","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Both hose handling Cranes Nuts and Bolts of platforms to be renewed. ","Deck - Machinery","General Appearance","Equipment Related",8.5,"Medium","Not Applicable","Not Applicable","Nut/ Bolts Renewed","2020-06-15",null,"Completed","2020-05-24","No",null,null,"Internal"]
[null,null,null,null,null,"99_8/3/2020 5:16:18 PM","2020-03-01","Defect","Ship Staff","Ship Staff Insp.","1C COT remote pressure sensor in SAAB Radar system not working","Miscellaneous","Cargo / Ballast Systems","Equipment Related",8.1300000000000008,"Medium","Not Applicable","Not Applicable","Renewed","2020-06-30",null,"Completed","2020-05-28","No",null,null,"Internal"]
[null,null,null,null,null,"99_29/5/2020 1:20:57 PM","2020-05-20","Defect","Ship Staff","Ship Staff Insp.","One section of Fresh water line found holed & heavily rusted","Deck - Pipe / Fittings","General Appearance","Equipment Related",11.4,"Very High","Not Applicable","Not Applicable","Fabricated & renewed","2020-05-31",null,"Completed","2020-05-29","No",null,null,"Internal"]
[null,null,null,null,null,"99_31/05/2020 08:37:58","2020-04-30","Defect","Ship Staff","Ship Staff Insp.","M.E UNIT # 4 & 5 fwd SIDE FUEL OIL H.P PIPE LEAKING FROM PUMP SIDE CONNECTION.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related",10.34,"High","Not Applicable","Not Applicable","M.E STOPPED, UNIT # 4 & 5 FWD SIDE H.P PIPE REPLACED WITH NEW SPARE PIPE.","2020-05-05",null,"Completed","2020-05-01","No",null,null,"Internal"]
[null,null,null,null,null,"99_31/05/2020 08:41:04","2020-04-30","Defect","Ship Staff","Ship Staff Insp.","M.E UNIT # 3 PUNCTURE VAVLE LEAKING FROM SEALING RING.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related",10.34,"High","Not Applicable","Not Applicable","M.E UNIT # 3 PUNCTURE VALVE AND SUCTION VALVE REMOVED FOR INSPECTION, FOUND SEALING RING OF SUCTION VALVE WAS BROKEN, SEALING RING OF BOTH PUNCTURE VALVE AND SUCTION VALVE RENEWED AND PUT BACK, ENGINE TRIED OUT, NO LEAKS OBSERVED.","2020-05-05",null,"Completed","2020-05-01","No",null,null,"Internal"]
[null,null,null,null,null,"99_31/05/2020 08:44:23","2020-05-03","Defect","Ship Staff","Ship Staff Insp.","AUX. ENGINE # 2 UNIT # 1 FUEL CONNECTION LEAKING.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related",null,null,"Not Applicable","Not Applicable","A.E # 2 ISOLATED, FUEL CONNECTION REMOVED, FOUND GASKET WAS BROKEN, SAME REPLACED AND CONNECTION PUT BACK. A.E TRIED OUT, NO LEAKS OBSERVED.","2020-05-03",null,"Completed","2020-05-03","No",null,null,"Internal"]
[null,null,null,null,null,"99_31/05/2020 08:49:33","2020-05-12","Defect","Ship Staff","Ship Staff Insp.","M.E Scavenge drain tank not draining to oily bilge tank, suspected drain valve chock.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related",null,null,"Not Applicable","Not Applicable","M.E scavenge drain tank man hole oepend, found sludge accumulation in the drain pipe, same cleared and tank cleaned. Manhole cover put back. ","2020-05-12",null,"Completed","2020-05-12","No",null,null,"Internal"]
[null,null,null,null,null,"99_31/05/2020 08:52:25","2020-05-09","Defect","Ship Staff","Ship Staff Insp.","Boiler # 1 feed water controller leaking from Gland.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related",10.3,"High","Not Applicable","Not Applicable","Boiler # 1 feed water gland packing removed, stem cleaned and new gland packing put in place. valve tried out, no leaks observed.","2020-05-15",null,"Completed","2020-05-13","No",null,null,"Internal"]
[null,null,null,null,null,"99_31/05/2020 08:55:40","2020-05-13","Defect","Ship Staff","Ship Staff Insp.","A.E # 2 starting air motor not getting disengaged while starting.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related",10.34,"High","Not Applicable","Not Applicable","A.E # 2 starting air solenoid valve removed and replaced with new spare valve. A.E tried out, motor mooving freely.","2020-05-13",null,"Completed","2020-05-13","No",null,null,"Internal"]
[null,null,null,null,null,"99_31/05/2020 08:58:00","2020-05-13","Defect","Ship Staff","Ship Staff Insp.","Incinerator refractory found damaged during inspection.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related",10.34,"High","Not Applicable","Not Applicable","Incinerator refractory patched up were ever it was broken.","2020-05-15",null,"Completed","2020-05-14","No",null,null,"Internal"]
[null,null,null,null,null,"99_31/05/2020 09:06:12","2020-05-17","Breakdown,Defect","Ship Staff","Ship Staff Insp.","Main Air Comp. # 2 H.P side air way cooler gasker leaking.","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related",10.34,"High","Not Applicable","Not Applicable","MAC # 2 isolated, end covers removed, both gaskets renewed, found one of the cooling water tube leaking, same pluged. End covers put back, comp. tried out. No leaks observed.","2020-05-18",null,"Completed","2020-05-17","No",null,null,"Internal"]
[null,null,null,null,null,"99_31/05/2020 09:09:08","2020-05-16","Defect","Ship Staff","Ship Staff Insp.","M.E unit # 1 & 5 CYl. head safety valves leking continuously.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related",10.34,"High","Not Applicable","Not Applicable","M.E unit # 1 & 5 safety valve removed, Curface cleaned, New safety valve put in place.","2020-05-17",null,"Completed","2020-05-17","No",null,null,"Internal"]
[null,null,null,null,null,"99_31/05/2020 09:12:44","2020-05-17","Defect","Ship Staff","Ship Staff Insp.","Boiler # 1 Boiler mounted feed water valve leaking from the Bonnet.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related",10.34,"High","Not Applicable","Not Applicable","Boiler # 1 depressurized, Valve bonnet removed, found damaged gasket, Gasket removed, suface cleaned. New gasket installed. Bonnet put back. Boiler pressed up, no leaks observed.","2020-05-18",null,"Completed","2020-05-18","No",null,null,"Internal"]
[null,null,null,null,null,"99_31/05/2020 09:15:27","2020-05-10","Defect","Ship Staff","Ship Staff Insp.","M.E air cooler # 1 chemical cleaning pipe have pin holes.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related",10.3,"High","Not Applicable","Not Applicable","M.E air cooler # 1 chemical cleaning pipe removed, Welded in workshop, Pipe pur back, no leaks observed.","2020-06-10",null,"Completed","2020-05-18","No",null,null,"Internal"]
[null,null,null,null,null,"99_31/05/2020 09:19:07","2020-05-15","Defect","Ship Staff","Ship Staff Insp.","HFO purifier # 1 water connection leaking from various placed due to corrosion.","E/R - Purifier","Eng. / Strg. Comp.","Equipment Related",10.3,"High","Not Applicable","Not Applicable","HFO purifier water connection removed, All corroded connections renewed. connection put back, no leaks observed.","2020-06-15",null,"Completed","2020-05-20","No",null,null,"Internal"]
[null,null,null,null,null,"99_31/05/2020 09:22:51","2020-05-19","Defect","Ship Staff","Ship Staff Insp.","Boiler # 2 Steam stop valve leaking from Bonnet.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related",10.34,"High","Not Applicable","Not Applicable","Both boiler steam stop valve closed, steam system depressurized, Valve bonned removed, damaged gasket removed and surface cleaned. New gasket installed, Bonnet put back, steam system put in use, no leaks observed.","2020-05-20",null,"Completed","2020-05-20","No",null,null,"Internal"]
[null,null,null,null,null,"99_31/05/2020 09:26:20","2020-05-15","Defect","Ship Staff","Ship Staff Insp.","A.E Fuel oil supply pump # 1 slight leak from mechanical seal.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related",10.34,"High","Not Applicable","Not Applicable","A.E supply pp # 1 isolated and dismantled, seal surface found damaged, Mech seal, oil seal and gaskets renewed. Pump boxed back and tried ouot, No leaks observed.","2020-05-30",null,"Completed","2020-05-22","No",null,null,"Internal"]
[null,null,null,null,null,"99_31/05/2020 09:29:56","2020-05-15","Defect","Ship Staff","Ship Staff Insp.","Main Fire pump # 1 overboard discharge valve was not moving and was stuck in open position.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related",null,null,"Not Applicable","Not Applicable","Main Fire pump # 1 over board discharge valve gland eased up, found stem rusted, same cleaned. New gland packing installed, Valve moving freely, no leaks observed.","2020-05-30",null,"Completed","2020-05-23","No",null,null,"Internal"]
[null,null,null,null,null,"99_31/05/2020 09:33:37","2020-05-25","Breakdown","Ship Staff","Ship Staff Insp.","Emcy. D.G not starting in auto/manual and indicating L.O low pressure alarm even in stop condition.","Critical Equip.","Eng. / Strg. Comp.","Equipment Related",10.34,"High","Not Applicable","Not Applicable","Emcy. D.G trouble shooting carried out, found ignition relay was malfunctioning. same replaced with new spare. D.G tried oout, working satisfactorily.","2020-05-25",null,"Completed","2020-05-25","No",null,null,"Internal"]
[null,null,null,null,null,"99_31/05/2020 09:37:14","2020-05-27","Defect","Ship Staff","Ship Staff Insp.","A.E fuel oil heater # 1 steam leaking from end cover.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related",10.3,"High","Not Applicable","Not Applicable","A.E heater isolated, end cover removed, Surface cleaned, Steam gasktes renewed. Cover put back. System put in use, no lekas observed.","2020-05-30",null,"Completed","2020-05-28","No",null,null,"Internal"]
[null,null,null,null,null,"99_17/5/2020 12:36:03 PM","2020-04-11","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Bottom of Gangway turntable to be de rusted and painted. ","Deck - Machinery","General Appearance","Inappropriate Procedure",5.47,"Medium","Not Applicable","Not Applicable","Derusting & painting Completed","2020-06-15",null,"Completed","2020-05-31","No",null,null,"Internal"]
[null,null,null,null,null,"99_23/3/2020 10:19:04 AM","2020-03-15","Defect","Ship Staff","Ship Staff Insp.","Lifebuoy hole not fitted with plugged. ","LSA / FFA","LSA / FFA Appliances","Equipment Related",5.31,"High","Not Applicable","Not Applicable","New lifebuoy received.","2020-05-31",null,"Completed","2020-05-26","No",null,null,"Internal"]
[null,null,null,null,null,"99_9/6/2020 5:12:29 PM","2020-06-01","Defect","Ship Staff","Ship Staff Insp.","Two fire hydrants on upper deck port & stbd found leaking","LSA / FFA","LSA / FFA Appliances","Equipment Related",null,null,"Not Applicable","Not Applicable","New valve renewed","2020-06-30",null,"Completed","2020-06-04","No",null,null,"Internal"]
[null,null,null,null,null,"99_17/4/2020 7:51:31 PM","2020-04-07","Defect","Ship Staff","Ship Staff Insp.","Port side Anchor chain stopper bar very hard to operate. Very hard to lift or lower","Deck - Pipe / Fittings","General Appearance","Equipment Related",9.1999999999999993,"Very High","Not Applicable","Not Applicable","Overhauled & Freed","2020-06-30",null,"Completed","2020-06-04","No",null,null,"Internal"]
[null,null,null,null,null,"99_9/6/2020 5:09:16 PM","2020-05-22","Defect","Ship Staff","Ship Staff Insp.","NO.2 Blue line Drop valve on main deck  found leaking","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related",8.11,"Medium","Not Applicable","Not Applicable","Seat ring renewed","2020-06-30",null,"Completed","2020-06-03","No",null,null,"Internal"]
[null,null,null,null,null,"99_23/3/2020 10:36:06 AM","2019-12-12","Defect","Ship Staff","Ship Staff Insp.","After taken over from other management helicopter equipment installed by 2 pcs of 25 Kg DCP & 2 Pcs of 10 Kg Co2 Fire extinguisher. Fire plan need to be Update and approve by Class.","LSA / FFA","LSA / FFA Appliances","Inappropriate Procedure",5.37,"Low","Not Applicable","Not Applicable"," Updated and approved by Class","2020-04-30",null,"Completed","2020-03-29","No",null,null,"Internal"]
[null,null,null,null,null,"99_21/5/2020 12:23:59 PM","2020-05-19","Defect","Ship Staff","Nav Audit / Verification","1 set of bridge window wipers not working","Navigation - Others","Navigation","Equipment Related",4.7,"High","Not Applicable","Not Applicable","Repaired, working satisfactory.","2020-06-19",null,"Completed","2020-05-30","No",null,null,"Internal"]
[null,null,null,null,null,"99_27/3/2020 1:18:23 AM","2020-01-01","Defect","Ship Staff","Ship Staff Insp.","Weather facsimile unit not receiving reports ","Navigation - Others","Navigation","Equipment Related",4.7,"High","Not Applicable","Not Applicable","Antenna connections cleaned & continuity to equipment checked. Equipment connections & wiring checked as per user manual, found in order. Equipment decomissioned as per office instructions.","2020-05-30",null,"Completed","2020-05-15","No",null,null,"Internal"]
[null,null,null,null,null,"99_13/04/2020 01:00:07","2020-04-03","Defect","Ship Staff","Ship Staff Insp.","FWG Ejector pump discharge valve body have pin holes in various places.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related",10.3,"Medium","Not Applicable","Not Applicable","FWG Ejector pump discharge valve replaced with new spare valve","2020-06-03","PERF200142","Completed","2020-04-17","No",null,null,"Internal"]
[null,null,null,null,null,"99_15/5/2020 8:17:52 AM","2020-04-26","Defect","Ship Staff","Ship Staff Insp.","M.E JACKET WATER PRE HEATER LEAKING FROM END COVER","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related",10.3,"Medium","Not Applicable","Not Applicable","M.E PRE HEATER END COVER TIGHTENED, NO LEAKS OBSERVED","2020-06-26",null,"Completed","2020-05-07","No",null,null,"Internal"]
[null,null,null,null,null,"99_15/5/2020 8:06:13 AM","2020-05-08","Defect","Ship Staff","Ship Staff Insp.","BOTH BOILER BOTTOM SOOT BLOW LINE HAVE SMALL LEAK.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related",10.3,"Medium","Not Applicable","Not Applicable","SOOT BLOW LINE GASKET RENEWED","2020-08-08",null,"Completed","2020-05-23","No",null,null,"Internal"]
[null,null,null,null,null,"99_13/04/2020 01:02:13","2020-04-03","Defect","Ship Staff","Ship Staff Insp.","FWG JCFW inlet pipe leaking from the flange connection.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related",10.3,"Medium","Not Applicable","Not Applicable","FWG JCFW inlet pipe flange gasket renewed.","2020-06-03",null,"Completed","2020-05-14","No",null,null,"Internal"]
[null,null,null,null,null,"99_30/04/2020 18:21:10","2020-03-29","Defect","Ship Staff","Ship Staff Insp.","FWG distillate pump leaking from the seal.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related",10.3,"Medium","Not Applicable","Not Applicable","FWG Distillate pump dismantled, seal cleaned and same seal put back as was in good condition. Pump tried out, no leaks observed.","2020-07-29",null,"Completed","2020-04-03","No",null,null,"Internal"]

{"sheet":"Calc","index":2,"n_rows":28,"n_cols":12,"rows_kept":28,"cut":false,"hidden":true,"merged":[]}
["Def_type","Def_cause","Equipments","VIQrefno","Observer_code"]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,"Dim itemSele As Long"]
[null,null,null,null,null,null,null,null,null,null,null,"   dim startRow as integer"]
[null,null,null,null,null,null,null,null,null,null,null,"   startRow=1"]
[null,null,null,null,null,null,null,null,null,null,null,"        For itemSele = 0 To ListBox1.ListCount - 1"]
[null,null,null,null,null,null,null,null,null,null,null,"        If ListBox1.Selected(itemSele) = True Then"]
[null,null,null,null,null,null,null,null,null,null,null,"        Worksheets(\"WorksheetName\").Range(\"A\" & startRow).Value = ListBox1.List(itemSele)"]
[null,null,null,null,null,null,null,null,null,null,null,"        startRow = startRow + 1"]
[null,null,null,null,null,null,null,null,null,null,null,"        End If"]
[null,null,null,null,null,null,null,null,null,null,null,"        Next"]
[null,null,null,null,null,null,null,null,null,null,null,"Dim LastRowA As String"]
[null,null,null,null,null,null,null,null,null,null,null,"        Dim itemSele As Long"]
[null,null,null,null,null,null,null,null,null,null,null,"       Dim startRow as integer"]
[null,null,null,null,null,null,null,null,null,null,null,"        LastRowA = ActiveSheet.Cells(Rows.count, \"A\").End(xlUp).row"]
[null,null,null,null,null,null,null,null,null,null,null,"        startQue = 0"]
[null,null,null,null,null,null,null,null,null,null,null,"        For itemSele = 0 To ListBox1.ListCount - 1"]
[null,null,null,null,null,null,null,null,null,null,null,"        For startRow = 1 To LastRowA"]
[null,null,null,null,null,null,null,null,null,null,null,"        If Worksheets(\"WorksheetName\").Range(\"A\" & startRow).Value = ListBox1.List(itemSele) Then"]
[null,null,null,null,null,null,null,null,null,null,null,"        ListBox1.Selected(itemSele) = True"]
[null,null,null,null,null,null,null,null,null,null,null,"        Exit For"]
[null,null,null,null,null,null,null,null,null,null,null,"        End If"]
[null,null,null,null,null,null,null,null,null,null,null,"        Next j"]
[null,null,null,null,null,null,null,null,null,null,null,"        Next"]
[null,null,null,null,null,null,null,null,null,null,null,"        End If"]

{"sheet":"Areaofobs","index":3,"n_rows":17,"n_cols":2,"rows_kept":17,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Cargo / Ballast Systems",11]
["Cert. & Docu.",2]
["Communication",6]
["Crew Management",3]
["Emgcy. Systems",13]
["Eng. / Strg. Comp.",14]
["General Appearance",15]
["Ice Opns.",17]
["ISM Related",7]
["ISPS Related",10]
["LSA / FFA Appliances",8]
["MARPOL Related",9]
["MLC Related",4]
["Mooring",12]
["Navigation",5]
["Structural Condn. / WT integrity ",16]

{"sheet":"Vessel_type","index":4,"n_rows":1,"n_cols":2,"rows_kept":1,"cut":false,"hidden":true,"merged":[]}
["Vessel_type","ID"]

{"sheet":"Deficiency_type","index":5,"n_rows":8,"n_cols":3,"rows_kept":8,"cut":false,"hidden":true,"merged":[]}
["TITLE","Type of deficiency_description","ID"]
["Breakdown",null,6]
["Critical Equipment",null,4]
["Defect",null,1]
["Guarantee Claim",null,8]
["Non Conformity",null,2]
["Observation",null,3]
["Other",null,7]

{"sheet":"VIQrefno","index":6,"n_rows":427,"n_cols":3,"rows_kept":427,"cut":false,"hidden":true,"merged":[]}
["VIQ_ref_no","Risk Value of observation","ID"]
["1.1","Low",8243]
["1.10","Low",8252]
["1.11","Low",8253]
["1.12","Low",8254]
["1.13","Low",8255]
["1.14","Low",8256]
["1.15","Low",8257]
["1.16","Low",8259]
["1.17","Low",8260]
["1.18","Low",8261]
["1.19","Low",8262]
["1.2","Low",8244]
["1.20","Low",8263]
["1.21","Low",8265]
["1.22","Low",8266]
["1.23","Low",8267]
["1.24","Low",8268]
["1.25","Low",8269]
["1.26","Low",8270]
["1.3","Low",8245]
["1.4","Low",8246]
["1.5","Low",8247]
["1.6","Low",8248]
["1.7","Low",8249]
["1.8","Low",8250]
["1.9","Low",8251]
["1.99","High",11258]
["10.1","Medium",8461]
["10.10","High",8470]
["10.11","Medium",8471]
["10.12","Very High",8472]
["10.13","Very High",8473]
["10.14","Medium",8474]
["10.15","Low",8475]
["10.16","Very High",8476]
["10.17","Very High",8477]
["10.18","High",8478]
["10.19","Very High",8479]
["10.2","Low",8462]
["10.20","High",8480]
["10.21","Medium",8481]
["10.22","Low",8482]
["10.23","Medium",8483]
["10.24","Low",8484]
["10.25","Very High",8485]
["10.26","High",8486]
["10.27","Medium",8487]
["10.28","Low",8488]
["10.29","Medium",8489]
["10.3","Medium",8463]
["10.30","High",8490]
["10.31","Very High",8491]
["10.32","Very High",8492]
["10.33","High",8493]
["10.34","High",8494]
["10.35","Very High",8495]
["10.36","Very High",8496]
["10.37","Medium",8497]
["10.38","Medium",8498]
["10.39","High",8499]
["10.4","High",8464]
["10.40","Medium",8500]
["10.41","Medium",8501]
["10.42","Medium",8502]
["10.43","Medium",8503]
["10.44","Medium",8504]
["10.45","Very High",8505]
["10.46","High",8506]
["10.47","Medium",8507]
["10.48","High",8508]
["10.49","Medium",8509]
["10.5","Low",8465]
["10.50","High",8510]
["10.51","Low",8511]
["10.52","Medium",8512]
["10.53","Medium",8513]
["10.54","High",8514]
["10.55","Low",8515]
["10.6","Very High",8466]
["10.7","Medium",8467]
["10.8","Medium",8468]
["10.9","Medium",8469]
["10.99","High",8516]
["11.1","High",8420]
["11.10","Medium",8429]
["11.11","Very High",8430]
["11.12","Low",8431]
["11.13","Low",8432]
["11.14","Medium",8433]
["11.15","Low",8434]
["11.16","Low",8435]
["11.17","Low",8436]
["11.2","Medium",8421]
["11.3","Medium",8422]
["11.4","Very High",8423]
["11.5","Medium",8424]
["11.6","Medium",8425]
["11.7","High",8426]
["11.8","Low",8427]
["11.9","Low",8428]
["11.99","High",8437]
["12.1","High",8438]
["12.10","High",8448]
["12.11","High",8449]
["12.12","High",8450]
["12.13","High",8451]
["12.14","High",8452]
["12.15","High",8453]
["12.16","High",8454]
["12.17","High",8455]
["12.18","High",8456]
["12.19","High",8457]
["12.2","High",8439]
["12.20","High",8458]
["12.21","High",8459]
["12.3","High",8441]
["12.4","High",8442]
["12.5","High",8443]
["12.6","High",8444]
["12.7","High",8445]
["12.8","High",8446]
["12.9","High",8447]
["12.99","High",8460]
["2.1","Very High",8296]
["2.1.9","Very High",11259]
["2.10","Medium",8304]
["2.11","Medium",8305]
["2.12","Low",8306]
["2.13","Low",8307]
["2.14","Low",8308]
["2.15","Low",8309]
["2.16","Medium",8310]
["2.2","Medium",8297]
["2.3","High",8295]
["2.4","Medium",8298]
["2.5","Medium",8299]
["2.6","Low",8300]
["2.7","High",8301]
["2.8","High",8302]
["2.9","Medium",8303]
["2.99","High",8311]
["3.1","High",8312]
["3.2","Very High",8313]
["3.3","High",8314]
["3.4","Low",8294]
["3.5","Medium",8315]
["3.6","High",8316]
["3.7","Very High",8317]
["3.8","Very High",8318]
["3.99","High",8319]
["4.1","High",8320]
["4.10","High",8329]
["4.11","Medium",8330]
["4.12","Very High",8331]
["4.13","Very High",8332]
["4.14","Very High",8333]
["4.15","Very High",8334]
["4.16","Very High",8335]
["4.17","Very High",8336]
["4.18","Very High",8337]
["4.19","Low",8338]
["4.2","Medium",8321]
["4.20","Very High",8339]
["4.21","High",8340]
["4.22","Low",8341]
["4.23","High",8342]
["4.24","High",8343]
["4.25","Low",8344]
["4.26","Low",8345]
["4.27","High",8346]
["4.3","Medium",8322]
["4.4","High",8323]
["4.5","Very High",8324]
["4.6","Medium",8325]
["4.7","High",8326]
["4.8","Medium",8327]
["4.9","Medium",8328]
["4.99","High",8347]
["5.1","Very High",8517]
["5.10","High",8526]
["5.11","Low",8527]
["5.12","Medium",8528]
["5.13","High",8529]
["5.14","Very High",8530]
["5.15","Medium",8531]
["5.16","Very High",8532]
["5.17","Very High",8533]
["5.18","High",8534]
["5.19","Medium",8535]
["5.2","Very High",8518]
["5.20","Medium",8536]
["5.21","Medium",8537]
["5.22","High",8539]
["5.23","Very High",8540]
["5.24","Very High",8541]
["5.25","Medium",8542]
["5.26","Medium",8543]
["5.27","Medium",8544]
["5.28","Very High",8545]
["5.29","High",8546]
["5.3","Low",8519]
["5.30","High",8547]
["5.31","High",8548]
["5.32","High",8549]
["5.33","High",8550]
["5.34","Low",8551]
["5.35","Medium",8552]
["5.36","Low",8553]
["5.37","Low",8554]
["5.38","High",8555]
["5.39","Very High",8556]
["5.4","High",8520]
["5.40","Very High",8557]
["5.41","Very High",8558]
["5.42","Medium",8559]
["5.43","High",8560]
["5.44","High",8561]
["5.45","Medium",8564]
["5.46","Medium",8565]
["5.47","Medium",8566]
["5.48","Medium",8567]
["5.5","Low",8521]
["5.6","Low",8522]
["5.7","Medium",8523]
["5.8","Medium",8524]
["5.9","Very High",8525]
["5.99","High",8568]
["6.1","Medium",8348]
["6.10","Low",8357]
["6.11","High",8358]
["6.12","Medium",8359]
["6.13","Low",8360]
["6.14","High",8361]
["6.15","High",8362]
["6.16","Very High",8363]
["6.17","Very High",8364]
["6.18","Medium",8365]
["6.19","Low",8366]
["6.2","High",8349]
["6.20","Medium",8367]
["6.21","High",8368]
["6.22","Medium",8369]
["6.3","Low",8350]
["6.4","High",8351]
["6.5","Medium",8352]
["6.6","Medium",8353]
["6.7","High",8354]
["6.8","High",8355]
["6.9","Low",8356]
["6.99","High",8370]
["7.1","High",8371]
["7.10","High",8380]
["7.11","High",8381]
["7.12","High",8382]
["7.13","Medium",8383]
["7.14","Medium",8384]
["7.15","High",8385]
["7.16","High",8386]
["7.17","High",8387]
["7.2","High",8372]
["7.3","Low",8373]
["7.4","Low",8374]
["7.5","Low",8375]
["7.6","Medium",8376]
["7.7","Low",8377]
["7.8","High",8378]
["7.9","High",8379]
["7.99","High",8388]
["8.1","Very High",8569]
["8.10","Very High",8578]
["8.100","Low",11227]
["8.101","Medium",11228]
["8.102","Low",11229]
["8.103","Low",11230]
["8.104","Low",11231]
["8.105","Medium",11232]
["8.106","Medium",11233]
["8.107","Low",11234]
["8.108","High",11235]
["8.109","Very High",11236]
["8.11","Medium",8579]
["8.110","High",11237]
["8.111","Medium",11238]
["8.112","High",11239]
["8.113","Medium",11240]
["8.114","Low",11241]
["8.115","High",11242]
["8.116","Medium",11243]
["8.117","Medium",11244]
["8.118","Medium",11245]
["8.119","High",11246]
["8.12","Medium",8580]
["8.120","High",11247]
["8.121","Medium",11248]
["8.122","High",11249]
["8.123","High",11250]
["8.124","Low",11251]
["8.125","High",11252]
["8.126","Medium",11253]
["8.127","Medium",11254]
["8.13","Medium",8581]
["8.14","Very High",8582]
["8.15","High",8583]
["8.16","Very High",8584]
["8.17","Low",8585]
["8.18","High",8586]
["8.19","High",8587]
["8.199","High",11255]
["8.2","Medium",8570]
["8.20","Medium",8588]
["8.21","High",8589]
["8.22","Very High",8590]
["8.23","Medium",8591]
["8.24","Medium",8592]
["8.25","Very High",8593]
["8.26","High",8594]
["8.27","Medium",8595]
["8.28","Medium",8596]
["8.29","High",8598]
["8.3","Very High",8571]
["8.30","High",8599]
["8.31","High",8600]
["8.32","Low",8601]
["8.33","Medium",8602]
["8.34","High",8603]
["8.35","Medium",8604]
["8.36","Medium",8605]
["8.37","High",8607]
["8.38","Medium",8608]
["8.39","Medium",8609]
["8.4","Medium",8572]
["8.40","High",8610]
["8.41","Medium",8611]
["8.42","Medium",8612]
["8.43","Very High",8613]
["8.44","High",8615]
["8.45","High",8616]
["8.46","Very High",8617]
["8.47","Very High",8618]
["8.48","Medium",8619]
["8.49","High",8620]
["8.5","Very High",8573]
["8.50","Medium",8621]
["8.51","Low",8622]
["8.52","Low",8623]
["8.53","Low",8624]
["8.54","High",8625]
["8.55","Low",11182]
["8.56","Medium",11183]
["8.57","Medium",11184]
["8.58","High",11185]
["8.59","High",11186]
["8.6","Medium",8574]
["8.60","High",11187]
["8.61","Medium",11188]
["8.62","Very High",11189]
["8.63","High",11190]
["8.64","Medium",11191]
["8.65","Low",11192]
["8.66","High",11193]
["8.67","High",11194]
["8.68","High",11195]
["8.69","Medium",11196]
["8.7","High",8575]
["8.70","Medium",11197]
["8.71","Very High",11198]
["8.72","Medium",11199]
["8.73","Medium",11200]
["8.74","High",11201]
["8.75","Medium",11202]
["8.76","Medium",11203]
["8.77","Medium",11204]
["8.78","Medium",11205]
["8.79","Medium",11206]
["8.8","Medium",8576]
["8.80","Medium",11207]
["8.81","Low",11208]
["8.82","Medium",11209]
["8.83","Low",11210]
["8.84","Low",11211]
["8.85","Medium",11212]
["8.86","Medium",11213]
["8.87","Medium",11214]
["8.88","Low",11215]
["8.89","High",11216]
["8.9","High",8577]
["8.90","High",11217]
["8.91","High",11218]
["8.92","Medium",11219]
["8.93","Low",11220]
["8.94","Low",11221]
["8.95","Medium",11222]
["8.96","Medium",11223]
["8.97","Low",11224]
["8.98","High",11225]
["8.99","Medium",11226]
["9.1","Low",8390]
["9.10","Medium",8399]
["9.11","Medium",8400]
["9.12","Medium",8401]
["9.13","Low",8402]
["9.14","Medium",8403]
["9.15","Medium",8404]
["9.16","High",8405]
["9.17","High",8406]
["9.18","Low",8407]
["9.19","Low",8408]
["9.2","Very High",8391]
["9.20","Medium",8409]
["9.21","Medium",8410]
["9.22","Low",8411]
["9.23","Low",8412]
["9.24","Medium",8413]
["9.25","Low",8414]
["9.26","Low",8415]
["9.27","Low",8416]
["9.28","Medium",8417]
["9.29","Low",8418]
["9.3","Very High",8392]
["9.4","High",8393]
["9.5","High",8394]
["9.6","Low",8395]
["9.7","Medium",8396]
["9.8","Medium",8397]
["9.9","Medium",8398]
["9.99","High",8419]

{"sheet":"Equipment_list","index":7,"n_rows":27,"n_cols":3,"rows_kept":27,"cut":false,"hidden":true,"merged":[]}
["TITLE","Equipment_list_description","ID"]
["Accommodation ",null,12]
["Cargo Mach.",null,13]
["Critical Equip.",null,16]
["Deck - Machinery",null,18]
["Deck - Mooring Machinery",null,15]
["Deck - Pipe / Fittings",null,20]
["Documentation",null,21]
["E/R - Air Comp.",null,8]
["E/R - Aux. Engine",null,4]
["E/R - Aux. Mach.",null,7]
["E/R - Boiler",null,5]
["E/R - Main Engine",null,3]
["E/R - Pipes/ valves & fittings",null,9]
["E/R - Purifier",null,6]
["Elect. Mach. & Equip.",null,10]
["Hull & Tanks",null,19]
["Inert Gas",null,14]
["LSA / FFA",null,17]
["Miscellaneous",null,22]
["Navigation - DGPS / EPFS / AIS",null,28]
["Navigation - ECDIS",null,25]
["Navigation - Echo Sounder / Speed Log",null,26]
["Navigation - GMDSS & Communication",null,23]
["Navigation - Others",null,11]
["Navigation - RADAR",null,24]
["Navigation - VDR / BNWAS",null,30]

{"sheet":"PSC_MOU","index":8,"n_rows":11,"n_cols":3,"rows_kept":11,"cut":false,"hidden":true,"merged":[]}
["TITLE","PSC_MOU_description","ID"]
["Asia and the Pacific",null,2]
["Caribbean",null,4]
["Europe and the North Atlantic",null,1]
["Latin America",null,3]
["The Black Sea region",null,6]
["The Indian Ocean",null,8]
["The Mediterranean",null,7]
["The Riyadh MoU",null,9]
["USCG",null,10]
["West and Central Africa",null,5]

{"sheet":"Inspection_type","index":9,"n_rows":11,"n_cols":2,"rows_kept":11,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Bunkering Audit",14]
["Engineering Audit",16]
["ISM Audit",2]
["ISPS Audit",3]
["IT Audit",10]
["MLC Audit",1]
["Mooring Audit",9]
["Nav Audit / Verification",8]
["Ship Staff Insp.",15]
["Suptd. Insp.",13]

{"sheet":"Deficiency_Cause","index":10,"n_rows":8,"n_cols":3,"rows_kept":8,"cut":false,"hidden":true,"merged":[]}
["TITLE","Deficiency_Cause_description","ID"]
["Behaviour Based",null,1]
["Equipment Related",null,4]
["External Factors",null,5]
["Human Error",null,7]
["Inappropriate Procedure",null,8]
["Industry Issue",null,6]
["Knowledge Based",null,3]

{"sheet":"Observer_code","index":11,"n_rows":3,"n_cols":3,"rows_kept":3,"cut":false,"hidden":true,"merged":[]}
["TITLE","Observer_code_description","ID"]
["Owner / Marine / Tech. Suptd.",null,3]
["Ship Staff",null,2]

{"sheet":"Status_code","index":12,"n_rows":6,"n_cols":3,"rows_kept":6,"cut":false,"hidden":true,"merged":[]}
["TITLE","Status_code_description","ID"]
["Completed",null,6]
["Deferred to D D",null,5]
["In progress",null,3]
["Not Started",null,2]
["Waiting spare",null,4]

{"sheet":"PSC_ref_no","index":13,"n_rows":19,"n_cols":2,"rows_kept":19,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Alarms",9]
["Cargo operations including equipment",7]
["Certificates & Documentation",2]
["Dangerous Goods",13]
["Emergency Systems",5]
["Fire safety",8]
["ISM",16]
["ISPS",17]
["Life saving appliances",12]
["MLC, 2006",18]
["Other",19]
["Pollution Prevention",15]
["Propulsion and auxiliary machinery",14]
["Radio communication",6]
["Safety of Navigation",11]
["Structural condition",3]
["Water/Weathertight condition",4]
["Working and Living Conditions",10]

{"sheet":"Risk_value_of_obs","index":14,"n_rows":1,"n_cols":2,"rows_kept":1,"cut":false,"hidden":true,"merged":[]}
["Risk Value of observation","ID"]

{"sheet":"Year","index":15,"n_rows":18,"n_cols":1,"rows_kept":18,"cut":false,"hidden":true,"merged":[]}
["Year"]
[2014]
[2015]
[2016]
[2017]
[2018]
[2019]
[2020]
[2021]
[2022]
[2023]
[2024]
[2025]
[2026]
[2027]
[2028]
[2029]
[2030]

{"sheet":"Month","index":16,"n_rows":13,"n_cols":1,"rows_kept":13,"cut":false,"hidden":true,"merged":[]}
["Month"]
["Jan"]
["Feb"]
["Mar"]
["Apr"]
["May"]
["Jun"]
["Jul"]
["Aug"]
["Sep"]
["Oct"]
["Nov"]
["Dec"]

{"sheet":"Date_","index":17,"n_rows":32,"n_cols":1,"rows_kept":32,"cut":false,"hidden":true,"merged":[]}
["Date"]
["01"]
["02"]
["03"]
["04"]
["05"]
["06"]
["07"]
["08"]
["09"]
[10]
[11]
[12]
[13]
[14]
[15]
[16]
[17]
[18]
[19]
[20]
[21]
[22]
[23]
[24]
[25]
[26]
[27]
[28]
[29]
[30]
[31]

{"sheet":"Sheet1","index":18,"n_rows":24,"n_cols":6,"rows_kept":24,"cut":false,"hidden":true,"merged":[]}
[]
[null,"ID","E",null,"Date Recorded",1]
[null,"UNIQUE ID","F",null,"Type of Deficiency",2]
[1,"Date Recorded","G",null,"Observer code",3]
["ignore","Vessel Type","H",null,"Type of Inspection",4]
[null,"Internal / External","I",null,"Description of Deficiency",5]
[null,"Drydock","J",null,"Equipment Categories",6]
[null,"Information Sharing","K",null,"Area of Observation",7]
[null,"Critical_item","L",null,"Deficiency Cause",8]
[null,"Deficiency Type","M",null,"VIQ Ref Number",9]
[null,"Deficiency Cause","N",null,"Risk Value of Obs",10]
[null,"Inspection Type","O",null,"PSC Ref Number",11]
[null,"Equipments","P",null,"PSC MOU ID",12]
[null,"VIQ Reference Number","Q",null,"Action Taken or Required",13]
[null,"Risk Value of the observation","R",null,"Target Date",14]
[null,"PSC Reference Number","S",null,"PO Ref No.",15]
[null,"PSC MOU","T",null,"Status Code",16]
[null,"Observer Code","U",null,"Date Completed",17]
[null,"Target Date","V",null,"Drydock",18]
[null,"Status Code","W",null,"Info Sharing",19]
[null,"Description of Deficiency","X",null,"Critical Item Flag",20]
[null,"Action taken / required","Y",null,"Audit Type",21]
[null,"PO ref no","Z"]
[null,"Date completed","AA"]

{"sheet":"Ship_information","index":19,"n_rows":2,"n_cols":3,"rows_kept":2,"cut":false,"hidden":true,"merged":[]}
["Ship_ID","Ship_Name","FILE_NAME"]
["99","PERFECT (26-12-2019)","99_1577777301290.xlsm"]

{"sheet":"External_Deficiency_type","index":20,"n_rows":5,"n_cols":3,"rows_kept":5,"cut":false,"hidden":true,"merged":[]}
["TITLE","Type of deficiency_description","ID"]
["Condn of Class / Memo",null,5]
["Defect",null,1]
["Non Conformity",null,2]
["Observation",null,3]

{"sheet":"External_Inspection_type","index":21,"n_rows":10,"n_cols":2,"rows_kept":10,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Flag State Insp.",5]
["ISM Audit",2]
["ISPS Audit",3]
["MLC Audit",1]
["Nav Audit / Verification",8]
["OM Insp. (Eg. SIRE / CDI etc.)",6]
["Others (Eg. Insurance etc.)",12]
["PSC Inspection",4]
["Terminal Insp.",11]

{"sheet":"External_Observer_code","index":22,"n_rows":7,"n_cols":3,"rows_kept":7,"cut":false,"hidden":true,"merged":[]}
["TITLE","Observer_code_description","ID"]
["Class Surveyor",null,4]
["FSC Inspector",null,5]
["Others (Eg. Insurance etc.)",null,9]
["PSC Insp.",null,6]
["SIRE / CDI Insp.",null,8]
["Terminal Insp.",null,7]

{"sheet":"Sheet Version","index":23,"n_rows":2,"n_cols":2,"rows_kept":2,"cut":false,"hidden":true,"merged":[]}
["Version","Title"]
["2.0","Version 2.0"]