{"text_format":"1","workbook":"xlsx","n_sheets":24,"sheets":["Mainsheet","Completed","Calc","Areaofobs","Vessel_type","Deficiency_type","VIQrefno","Equipment_list","PSC_MOU","Inspection_type","Deficiency_Cause","Observer_code","Status_code","PSC_ref_no","Risk_value_of_obs","Year","Month","Date_","Sheet1","Ship_information","External_Deficiency_type","External_Inspection_type","External_Observer_code","Sheet Version"],"not_rendered":{"charts":0,"images":6,"macros":1,"external_links":0,"defined_names":12,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Mainsheet","index":0,"n_rows":47,"n_cols":28,"rows_kept":47,"cut":false,"hidden":false,"merged":[[10,8,10,9],[10,12,10,13],[12,6,12,27],[8,6,8,27]]}
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,"Defect - Damage Monitoring Sheet"]
[]
[null,null,null,null,null,null,null,"Date of Report","12-Jun-2020",null,null,"Ship Name","PROMOTER (06-06-2020)"]
[]
[null,null,null,null,null,null,"VERSION : 2.0"]
[]
[]
[]
[null,null,null,null,"ID","UNIQUE ID","Date Recorded","Type of Deficiency","Observer code","Type of Inspection","Description of Deficiency","Equipment Categories","Area of Observation","Deficiency Cause","VIQ Ref Number","Risk Value of Obs","PSC Ref Number","PSC MOU ID","Action Taken or Required","Target Date","PO Ref No.","Status Code","Date Completed","Drydock","Info Sharing","Critical Item","Audit Type","Superintendent Remarks"]
[null,null,null,null,8310,"100_14-12-2019 12:12:45","2019-12-02","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","As per the running hours provided by previous Management # 6 unit decarb will be due in 1200 hours and # 7 unit decarb will be due in 2700 hours. ","E/R - Main Engine","Eng. / Strg. Comp.","External Factors",10.32,"Very High","Not Applicable","Not Applicable","Consult with technical department, upon sighting the performance and condition and spares, and plan the job as required.Also As per Maker new Cermeted coated Piston rings to be fitted for all the unit for new low sulphur fuels.","2020-08-31","PROM200004","Deferred to D D",null,"Yes","No","No","Internal"]
[null,null,null,null,8312,"100_14-12-2019 12:18:55","2019-12-02","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","# 1 Main engine and Aux engine fuel oil supply and booster pump(Both The Pumps) making abnormal sound, need to overhaul all  pumps","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","RO raised for new IMO Pumps for running on VLSFO, LSMGO.  RO number PROM200124","2020-08-31","PROM200124","Waiting spare",null,"No","No","No","Internal","There is no RO mentioned in this report. What is vessel plan of action as this is long pending."]
[null,null,null,null,8314,"100_14-12-2019 12:28:14","2019-12-02","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Steering Gear System having Leaks from all four rams","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","(RAM no. 1 fwd stbd) & (RAM no. 2 Fwd port) 2 ltrs/day , (RAM no. 3Aft stbd) &  (RAM no. 4 Aft port) 3 ltrs/day ,    \n\nJOB already included in DD spec","2020-08-30","","Deferred to D D",null,"Yes","No","No","Internal","Let us know how much leakage is there from each ram & has job included in DD  specs."]
[null,null,null,null,8315,"100_14-12-2019 12:31:59","2019-12-02","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Steering gear motor starboard side making abnormal Noise.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Vessel has spare bearing and will Carry out overhauling of motor as next opportunity","2020-08-30","","In progress",null,"No","No","No","Internal","Confirm vessel has required bearings for overhaul of motor, plan it & carryout asap."]
[null,null,null,null,8327,"100_17-12-2019 06:43:16","2019-12-04","Defect","Ship Staff","Ship Staff Insp.","Aux engine Fuel oil inlet and Outlet flowmeters not working.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","New flowmeters on order.","2020-07-30","PROM200026","Waiting spare",null,"No","No","No","Internal","It is being arranged by NGM, will check & revert."]
[null,null,null,null,8328,"100_17-12-2019 06:50:02","2019-12-04","Defect","Ship Staff","Ship Staff Insp.","Vacuum condenser cooling sea water pump suction filter body in holed.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.31","Very High","","","Tempapory repairs carried out. The filter casing is wasted in many parts inisde.                            Requisition no. PROM200123 raised for new filter casing","2020-08-31","PROM200123 ","Deferred to D D",null,"Yes","No","No","Internal","Vsl to raise RO for supply of new filter supported with relevant drawings."]
[null,null,null,null,8336,"100_19/12/2019 18:15:49","2019-12-04","Defect","Ship Staff","Ship Staff Insp.","Stbd lifeboat winch brake shoe pads worn out.","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.28","Very High","","","Defect raised as per recommendation in Last Lifeboat Service. Shoe pad replacement to be done in next Lifeboat annual service","2020-12-04","","Deferred to D D",null,"No","No","No","Internal","What is PO no for brake shoe pads & reason for not completing this job till date."]
[null,null,null,null,8370,"100_Wed Jun 12 2019 15:13:14 GMT+0000 (Coordinated Universal Time)","2019-12-04","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Various protection plates/covers for pipes on main deck wasted.","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","Equipment Related","11.5","Medium","","","New plates/covers to be fabricated and fitted","2020-08-31","","Deferred to D D",null,"Yes","No","No","Internal"]
[null,null,null,null,8371,"100_Wed Jun 12 2019 15:18:12 GMT+0000 (Coordinated Universal Time)","2019-12-04","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Various angle bar supports on main deck wasted.","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","Inappropriate Procedure","11.5","Medium","","","New angle bars to be fabricated and fitted","2020-08-31","","Deferred to D D",null,"Yes","No","No","Internal"]
[null,null,null,null,8304,"100_13/12/2019 03:39:23","2019-12-05","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Crew & officer smoke rooms sofas in poor condition","Accommodation","MLC Related","External Factors","11.13","Low","","","Job has been added in DD specs","2020-08-31","","Deferred to D D",null,"No","No","No","Internal","Defect to be transferred to DD & DD specs for same to be raised & submitted to office."]
[null,null,null,null,8305,"100_13/12/2019 03:43:59","2019-12-05","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Bridge very hot & need to be equipped with 2 tons split air condition to avoid damage to electronic components","Accommodation","MLC Related","External Factors","11.16","Low","","","RO  raised for new air con","2020-08-31","PROM 200033","Waiting spare",null,"No","No","No","Internal","Not available in USA, will be connected at next oppertunity."]
[null,null,null,null,8329,"100_17-12-2019 06:52:34","2019-12-05","Defect","Ship Staff","Ship Staff Insp.","IG scrubber cooling sea water Pump Suction Filter having soft patches all over the filter casing","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.31","Very High","","","To change the filter casing by fabrication new suction filtercasing. Requisition no. PROM200123 raised for new casing","2020-08-31","PROM200123","Deferred to D D",null,"Yes","No","No","Internal","RO to be raised for supply of filter casing supported with relevant dimensional drawing."]
[null,null,null,null,8337,"100_19/12/2019 18:22:10","2019-12-05","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","All mooring winch brake bands are rusted and not os stainless steel material.","Deck - Mooring Machinery","Mooring","Equipment Related","9.15","Medium","","","Bands to be derusted temporarily and same to be renewed with SS bands","2020-08-31","","Deferred to D D",null,"Yes","No","No","Internal"]
[null,null,null,null,8344,"100_20/12/2019 00:02:08","2019-12-07","Defect","Owner / Marine / Tech. Suptd.,Ship Staff","Suptd. Insp.","Suez canal light cable penetration pipe wasted","Deck - Pipe / Fittings","General Appearance","Inappropriate Procedure","11.11","Very High","","","Pipe to be crop & renew","2020-10-06","","Deferred to D D",null,"No","No","No","Internal"]
[null,null,null,null,8335,"100_19/12/2019 16:25:49","2019-12-08","Defect","Ship Staff","Ship Staff Insp.","Many in use mooring ropes condition found bad.","Miscellaneous,Deck - Mooring Machinery","Mooring","Inappropriate Procedure","9.5","High","","","New mooring ropes to be ordered and deteriorated ones to be discarded. RO raised","2020-07-31","PROM 200082","Waiting spare",null,"No","No","No","Internal","Will be connected at next convenient port."]
[null,null,null,null,8346,"100_20/12/2019 00:20:22","2019-12-09","Defect","Ship Staff","Ship Staff Insp.","Some of the mooring tails in use are more then 18 months in service and overall condition found deteriorated.","Miscellaneous","Mooring","Inappropriate Procedure","9.5","High","","","New rope tails ordered.","2020-08-31","PROM 200082","Waiting spare",null,"No","No","No","Internal","Will be connected at next convenient port."]
[null,null,null,null,8353,"100_20/12/2019 01:03:21","2019-12-12","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Channel of most of the valve hydraulic boxes on deck are corroded.","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","Equipment Related","11.5","Medium","","","Box channels to be renewed","2020-08-31","","Deferred to D D",null,"Yes","No","No","Internal"]
[null,null,null,null,8354,"100_20/12/2019 01:06:26","2019-12-12","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Deep grooving observed on most of the closed chokes","Deck - Pipe / Fittings","Mooring","Equipment Related,Inappropriate Procedure","9.18","Low","","","Job added in DD specs","2020-08-31","","Deferred to D D",null,"No","No","No","Internal","Make temporary repairs to avoid vetting observation. Since hot work is involved & permanent repairs can't be done without gas free, postpone job to DD & raise DD specs."]
[null,null,null,null,8350,"100_20/12/2019 00:49:56","2019-12-18","Defect","Ship Staff","Ship Staff Insp.","Hydraulic oil loss from VRCS observed during cargo operations.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related",11.4,"Very High","Not Applicable","Not Applicable","All ballast and Cargo valves tried out locally using hand pump.Leak found on shut side for B2 (Bottom crossover) in Box NO. R2. For 6ss (6 stbd Stripping valve)in  Box NO.R7. Box No.R1 to R7 tried out individually using hydraulic pump, Found oil drop for Box No.R4. Box NO. R2,R4 & R7 kept isolated during cargo operations to minimize oil loss. Office concurrence required for further repairs which will require de-slopping as well.","2020-08-31",null,"In progress",null,"No","No","No","Internal"]
[null,null,null,null,12084,"100_9/3/2020 5:15:16 AM","2020-02-02","Defect,Observation","Ship Staff","Ship Staff Insp.","Fire GS pump Outlet Manifold Found having Pin Hole","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related",10.31,"Very High","Not Applicable","Not Applicable","Tempaproy repairs with Wencon carried out. Entire pipe manifold to be renewed. Manifold job included in DD specs.Material RO PROM200126 raised","2020-08-28"," PROM200126","Deferred to D D",null,"Yes","No","No","Internal","Confirm pump & line valves are holding as need to carryout permanent repairs. Pls confirm vessel has material to carryout permanent repairs."]
[null,null,null,null,12085,"100_4/3/2020 3:05:49 AM","2020-02-20","Defect,Observation","Ship Staff","Ship Staff Insp.","Engine Room all blower casing found wasted at various places, Also full of rust.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Temparory repairs carried out with devcon and area build up applied paint. De rusting of blowers from isnide carried out. New Casing to fitted at DD or Sections to be fabricated from shore workshop & to be supplied to vessel.","2020-08-28","","Deferred to D D",null,"Yes","No","No","Internal"]
[null,null,null,null,12086,"100_9/3/2020 5:11:32 AM","2020-02-29","Breakdown,Defect","Ship Staff","Ship Staff Insp.","Forward air horn found defective","Navigation - Others","Navigation","Equipment Related",4.2,"Medium","Not Applicable","Not Applicable","Renewed diaphragm and soleniod valve replaced with AFT air horn, solenoid valve, Now Forward horn working but AFT horn Inoperational. Received the RO at Aruba and vessel plans to change on 17th July 2020","2020-08-31","PROM200058","In progress",null,"No","No","No","Internal","Spares sourced & will be connected at next convenient port."]
[null,null,null,null,12087,"100_20/3/2020 4:46:38 AM","2020-03-02","Defect","Ship Staff","Ship Staff Insp.","Aux cooling SW pump # 1 and # 2  Suction Valve and dischagrevalaves not holding.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","PROM200126 , after valves received job to be carried out by using alternate cooling arrangement for AE coolers & closing both sea chest, Job included in DD specs","2020-08-28","PROM200126 ","Deferred to D D",null,"No","No","No","Internal","Pls confirm  vsl sea chest valves are holding."]
[null,null,null,null,12088,"100_3/4/2020 4:16:05 AM","2020-03-02","Observation","Ship Staff","Ship Staff Insp.","Engine Room Workshop Lathe machine and Bench Grinder doesnt have emergency stop.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.3","Medium","","","RO raised . Awaiting Spare","2020-07-31","PROM200068","Waiting spare",null,"No","No","No","Internal","Spares sourced & will be connected to vessel at next convenient port."]
[null,null,null,null,12089,"100_17/4/2020 12:49:38 AM","2020-03-02","Other","Ship Staff","Ship Staff Insp.","Deck Seal Pump # 1 Suction and Discharge Valve not holding and completely Closing","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.3","Medium","","","PROM200126 , after valves received job to be carried out by using alternate cooling arrangement for AE coolers & closing both sea chest, Job included in DD specs","2020-08-28","PROM200126","Deferred to D D",null,"Yes","No","No","Internal"]
[null,null,null,null,12091,"100_17/4/2020 12:45:51 AM","2020-04-02","Other","Ship Staff","Ship Staff Insp.","IG Scrubber Cooling SW pump Suction Valve not closing Completely/ Valve not Holding","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.3","Medium","","","PROM200126 , after valves received job to be carried out by using alternate cooling arrangement for AE coolers & closing both sea chest.Job Also Included in DD Specs.","2020-08-28","PROM200126","Deferred to D D",null,"Yes","No","No","Internal","Pls confirm vessel has spare valve for replacement. If available, same can be carried out by having blackout with RA in place. Kindly revert."]
[null,null,null,null,12094,"100_16/5/2020 5:31:30 AM","2020-04-24","Defect,Observation","Ship Staff","Ship Staff Insp.","Stbd Lifeboat Air hose to Pressure guage found leaking from the coupling.","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.15","Medium","","","To replace with new spare hose. Part number details are not available in manual. ","2020-08-31","PROM200109","Waiting spare",null,"No","No","No","Internal","Unable to source hoses till date. Kindly revert if it has some part no from Instruction Manyual."]
[null,null,null,null,12092,"100_22/5/2020 10:41:12 PM","2020-05-01","Observation","Ship Staff","Ship Staff Insp.","VRCS No.2 Hydraulic Pump  Making Abnormal While starting.","Miscellaneous","Cargo / Ballast Systems","Equipment Related",11.4,"Very High","Not Applicable","Not Applicable","Motor has been overhauled on 22 May 2020,coupling ckecked found ok , Piston pump inspected found parts worn out. New Pump On order.","2020-08-31","PROM200127","Waiting spare",null,"No","No","No","Internal","Job is supposed to be complete by 31st May & now reflecting overdue, kindly let us know reason for not carrying out job. Also insert VIQ Reference No as same not done. Vessel to raise RO."]
[null,null,null,null,12093,"100_16/5/2020 5:13:44 AM","2020-05-09","Defect","Ship Staff","Ship Staff Insp.","Bunker Line leaking and wasted at various places forward of accomdation from aft manifold to aft isloation valve and engine room isolation valve.","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","Equipment Related","6.7","High","","","PROM200126 pipes, bends  & flanges material requisition raised, after receiving to fabricate bunker line.Manifold job included in DD specs","2020-08-28","PROM200126 ","Deferred to D D",null,"Yes","No","No","Internal"]
[null,null,null,null,null,"100_17/7/2020 5:17:50 AM","2020-07-06","Critical Equipment,Non Conformity","Ship Staff","Ship Staff Insp.","Incinerator ID Fan Impeller Found Damaged. Casing Found Damged. Shaft Found Bend.","Critical Equip.","Eng. / Strg. Comp.","Equipment Related",10.3,null,"Not Applicable","Not Applicable","Fan Impeller,Shaft, Bearings ,Inlet Cone All removed and Casing Repaired. RO Rasied For All the Parts.","2020-09-30","PROM 200145","Waiting spare",null,"No",null,null,"Internal"]

{"sheet":"Completed","index":1,"n_rows":120,"n_cols":28,"rows_kept":120,"cut":false,"hidden":false,"merged":[[10,8,10,9],[10,12,10,13],[12,6,12,27],[8,6,8,27]]}
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,"Defect - Damage Monitoring Sheet"]
[]
[null,null,null,null,null,null,null,"Date of Report","12-Jun-2020",null,null,"Ship Name","PROMOTER (06-06-2020)"]
[]
[null,null,null,null,null,null,"VERSION : 2.0"]
[]
[]
[]
[null,null,null,null,"ID","UNIQUE ID","Date Recorded","Type of Deficiency","Observer code","Type of Inspection","Description of Deficiency","Equipment Categories","Area of Observation","Deficiency Cause","VIQ Ref Number","Risk Value of Obs","PSC Ref Number","PSC MOU ID","Action Taken or Required","Target Date","PO Ref No.","Status Code","Date Completed","Drydock","Info Sharing","Critical Item","Audit Type","Superintendent Remarks"]
[null,null,null,null,8311,"100_14-12-2019 12:15:41","2019-12-02","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Both Camshaft pump Making Abnormal noise while engine standstill.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Pump Motors Overhauled.No abnormal sound","2020-03-31","","Completed","2020-03-17","No","No","No","Internal"]
[null,null,null,null,8313,"100_14-12-2019 12:22:05","2019-12-02","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Fresh Water Generator china make producing reported 10 tons per day against the capacity of 30 tons per day","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Fresh water generator condenser and evaporator  cleaned manaually. Evaporater Side Chemical CIP Carried out. Distallate Pump opened up and impeller checked and cleaned. Brine side flap valve opened and cleaned. Salinmometer cell cleaned.The Production has come up to 17-18 tons a Day. Due to short voayges and CP speed not able to test at full speed.","2020-01-31","","Completed","2020-01-25","No","No","No","Internal"]
[null,null,null,null,8316,"100_14-12-2019 12:36:12","2019-12-02","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Area Above FD fan poorly lighted and poorly maintained\t","Miscellaneous","Eng. / Strg. Comp.","External Factors,Inappropriate Procedure","10.32","Very High","","","Cleaned, Painted. Light fixtures need to increased in Dry dock","2020-05-31","","Completed","2020-03-24","No","No","No","Internal"]
[null,null,null,null,8317,"100_14-12-2019 12:39:58","2019-12-02","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Engine room bulkhead with dirt depoists","Miscellaneous","Eng. / Strg. Comp.","External Factors","10.32","Very High","","","Cleaned and Painted as required.","2020-04-30","","Completed","2020-03-30","No","No","No","Internal"]
[null,null,null,null,8361,"100_14-12-2019 12:00:07","2019-12-02","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Low pressure trip for ME LO and Canshaft LO Bypassed by previous crew , investigation to inprogress and pinpoint cause for defect. engine room to be kept manned\t","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","ME alarms and trips inhibited from ECR by inhibit push button. After removing Inhibit and trying out the alarms found alarms and trips for M|E saftey system working satisfactorily.","2019-12-10","","Completed","2019-12-08","No","No","No","Internal"]
[null,null,null,null,8362,"100_14-12-2019 12:24:51","2019-12-02","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Incinerator Flame Failure not operational","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","Changed relay and found flame faliure working satisfactorliy","2019-12-10","","Completed","2019-12-06","No","No","No","Internal"]
[null,null,null,null,null,"100_14-12-2019 12:04:00","2019-12-02","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","No instrument provided for recording ME and aux engine performance","E/R - Aux. Engine,E/R - Main Engine","Eng. / Strg. Comp.","Behaviour Based,Equipment Related,External Factors",10.32,"Very High","Not Applicable","Not Applicable","Vessel Received the spare at aruba on 15th July 2020. Performance will be recorded","2020-08-30","PROM200017","Completed","2020-07-16","No",null,null,"Internal"]
[null,null,null,null,8318,"100_14-12-2019 12:42:19","2019-12-03","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Area behind Cascade tank dirty","Miscellaneous","Eng. / Strg. Comp.","External Factors","10.32","Very High","","","Cleaning Completed, Painted the Area Completely with paint received.","2020-03-31","","Completed","2020-03-25","No","No","No","Internal"]
[null,null,null,null,8319,"100_14-12-2019 12:50:05","2019-12-03","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Area below hyrdophore and OWS dirty","Miscellaneous","Eng. / Strg. Comp.","External Factors","10.32","Very High","","","Cleaned Completely, Painted as required.","2020-03-31","","Completed","2020-03-24","No","No","No","Internal"]
[null,null,null,null,8320,"100_14-12-2019 12:58:18","2019-12-03","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","# 1 LO purifier slight leak from top of hood","E/R - Purifier","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","O-ring changed when purifer opened up for bowl cleaning- 2000 hrs routine.","2019-12-31","","Completed","2019-12-22","No","No","No","Internal"]
[null,null,null,null,8321,"100_14-12-2019 13:03:06","2019-12-03","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Starboard hydraulic valve block panel having leak from 102 and 103 valve blocks","Deck - Machinery","Mooring","Equipment Related","6.4","High","","","Leak rectified.","2020-04-30","","Completed","2020-02-26","No","No","No","Internal"]
[null,null,null,null,8322,"100_14-12-2019 13:06:31","2019-12-03","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Deak seal pumps outlet pipe having leaks from pipe and flanges.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","",""," Renew flange gasket and bolts.","2020-03-31","","Completed","2020-01-31","No","No","No","Internal"]
[null,null,null,null,8363,"100_14-12-2019 12:46:02","2019-12-03","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ME area above scavenge mainfold on aft starboard side oil/dirt","E/R - Main Engine","Eng. / Strg. Comp.","External Factors","","","","","Area cleaned.","2019-12-31","","Completed","2019-12-12","No","No","No","Internal"]
[null,null,null,null,8364,"100_14-12-2019 12:54:00","2019-12-03","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Both LO Purifier oil inlet temperature maintained at 85 deg cent against 90 ~ 95 deg cent","E/R - Purifier","Eng. / Strg. Comp.","Equipment Related","","","","","Heater setting increased now maintaining 90 deg cent.","2019-12-10","","Completed","2019-12-08","No","No","No","Internal"]
[null,null,null,null,8366,"100_14-12-2019 13:20:45","2019-12-03","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Oxygen/ acetylene cylinders stored on wood","Miscellaneous","Eng. / Strg. Comp.","External Factors,Human Error","","","","","Wood removed and new metal stand fabricated and bottles placed on stand.","2019-12-10","","Completed","2019-12-05","No","No","No","Internal"]
[null,null,null,null,8295,"100_Fri Jul 12 2019 14:54:03 GMT+0000 (Coordinated Universal Time)","2019-12-04","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Fwd ETA in poor condition","Documentation","Cargo / Ballast Systems","Inappropriate Procedure","9.28","Medium","","","ETA dersuted and painted.","2020-03-04","","Completed","2020-04-20","No","No","No","Internal"]
[null,null,null,null,8323,"100_14-12-2019 13:13:50","2019-12-04","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ows inlet and outlet pipes lagging dirty","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Lagging Renewed and painted as required","2020-01-31","","Completed","2020-01-20","No","No","No","Internal"]
[null,null,null,null,8324,"100_14-12-2019 13:24:02","2019-12-04","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Emergency fire pump and steering gear drain valave located at aft bottom part near forward stearn tube seal tank, frozen /rusted.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","External Factors","","","","","Both the drain Valves opened up and overhauled.Gasket renewed. Now operating properly.","2020-01-31","","Completed","2020-01-28","No","No","No","Internal"]
[null,null,null,null,8325,"100_14-12-2019 13:26:24","2019-12-04","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Aft stbd winch having slight leakage from flange","Deck - Mooring Machinery","Mooring","Equipment Related","9.14","Medium","","","Flange bolt tightened .Confirmed during operations no leakage.","2020-03-29","","Completed","2020-01-10","No","No","No","Internal"]
[null,null,null,null,8326,"100_14-12-2019 13:29:14","2019-12-04","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Dirty lagging of pipes in lobby, vegetable room and linen store","Accommodation","General Appearance","External Factors","11.5","Medium","","","Dirty lagging renewed and painting carried out.","2020-08-31","","Completed","2020-05-21","No","No","No","Internal","Update reason for not starting job."]
[null,null,null,null,8359,"100_Wed Jun 12 2019 17:44:28 GMT+0000 (Coordinated Universal Time)","2019-12-04","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Loose earth cable for wilden pumps on deck.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","Earthing cable fitted properly in place and clamping area paint removed.","2019-12-07","","Completed","2019-12-06","No","No","No","Internal"]
[null,null,null,null,8365,"100_14-12-2019 13:10:01","2019-12-04","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Vacuum condensor pump having leak marks at shaft area","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Gland tightened and old leak marks removed. found no leaks from shaft area.","2019-12-31","","Completed","2019-12-13","No","No","No","Internal"]
[null,null,null,null,8372,"100_Wed Jun 12 2019 15:25:30 GMT+0000 (Coordinated Universal Time)","2019-12-04","Defect","Ship Staff","Ship Staff Insp.","Port and stbd side lifeboat rowing port cover securing hinge broken","LSA / FFA","Safety / LSA / FFA","Equipment Related,External Factors,Inappropriate Procedure","5.27","Medium","","","New cover fabricated for port side lifeboat and stbd side lifeboat cover repaired.","2019-12-08","","Completed","2019-12-06","No","No","No","Internal"]
[null,null,null,null,8373,"100_Wed Jun 12 2019 15:38:58 GMT+0000 (Coordinated Universal Time)","2019-12-04","Defect","Ship Staff","Ship Staff Insp.","Port side gangway lower platform stauchion base pipe broken","Deck - Machinery","Structural Condn. / WT integrity ","Behaviour Based,Equipment Related,External Factors","5.47","Medium","","","New stauchion pipe fabricated and fitted.","2019-12-07","","Completed","2019-12-05","No","No","No","Internal"]
[null,null,null,null,8374,"100_Fri Dec 06 2019 17:03:49 GMT+0000 (Coordinated Universal Time)","2019-12-04","Defect","Ship Staff","Ship Staff Insp.","One no. UTI found with tape detached/broken from sensor and one no. UTI tape kinked at various locations.","Cargo Mach.,Critical Equip.","Cargo / Ballast Systems","Equipment Related,Inappropriate Procedure","8.22","Very High","","","Serivicing and calibration of UTI's carried out, New tape received.","2020-04-29","","Completed","2020-04-15","No","No","No","Internal"]
[null,null,null,null,8375,"100_Wed Jun 12 2019 17:37:43 GMT+0000 (Coordinated Universal Time)","2019-12-04","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Broken round bar at end of port pilot embarkation platform near ship side.","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","Equipment Related,Inappropriate Procedure","5.47","Medium","","","Platform dismantled and repaired","2020-08-31","","Completed","2020-05-23","No","No","No","Internal"]
[null,null,null,null,8292,"100_Fri Jul 12 2019 11:34:21 GMT+0000 (Coordinated Universal Time)","2019-12-05","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Toilet tiles in majority of cabins found broken.","Accommodation","MLC Related","Inappropriate Procedure","11.13","Low","","","All broken tiles of crew cabins renewed as required. ","2020-06-30","","Completed","2020-06-06","No","No","No","Internal"]
[null,null,null,null,8293,"100_Fri Jul 12 2019 11:36:49 GMT+0000 (Coordinated Universal Time)","2019-12-05","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Shower curtains missing inside few cabin toilets.","Accommodation","MLC Related","Inappropriate Procedure","11.13","Low","","","New shower curtains were installed in cabins.","2020-01-04","","Completed","2020-01-03","No","No","No","Internal"]
[null,null,null,null,8296,"100_13/12/2019 02:13:40","2019-12-05","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Midship stores, engine stores, deck & galley stores poorly arranged.","Miscellaneous","General Appearance","Behaviour Based,Inappropriate Procedure","5.11","Low","","","All stores cleaned & arranged and inventories taken.","2020-01-31","","Completed","2020-01-29","No","No","No","Internal"]
[null,null,null,null,8298,"100_13/12/2019 02:42:38","2019-12-05","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Water weeping marks observed on both anchor chain washing lines in forecastle store.","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","Equipment Related","9.2","Very High","","","Leak rectified.","2020-08-31","","Completed","2020-05-25","No","No","No","Internal"]
[null,null,null,null,8299,"100_13/12/2019 02:50:06","2019-12-05","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Toilet bowl on CCR deck broken & blocked","Accommodation","MLC Related","External Factors","11.13","Low","","","Repairs carried out and WC made operational.","2020-01-30","","Completed","2020-01-30","No","No","No","Internal"]
[null,null,null,null,8300,"100_13/12/2019 03:03:44","2019-12-05","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Missing curtains/bed lights in crew cabins.","Accommodation","MLC Related","External Factors,Inappropriate Procedure","11.13","Low","","","Curtains cleaned. Lights renewal completed. Tiles renewed as per other job in defect list. ","2020-06-30","","Completed","2020-06-06","No","No","No","Internal"]
[null,null,null,null,8302,"100_13/12/2019 03:29:10","2019-12-05","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Broken floor tiles in Galley.","Accommodation","MLC Related","External Factors","11.13","Low","","","Broken floor tiles in Galley to be replaced","2020-03-03","","Completed","2020-02-26","No","No","No","Internal"]
[null,null,null,null,8303,"100_13/12/2019 03:34:58","2019-12-05","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Missing entertain system in Crew smoke room, Chief Engineer cabins. Officer smoke room entertainment system in poor condition.","Accommodation","MLC Related","External Factors","11.16","Low","",""," Entertainment systems received for Crew and officer smoke, also for Chief Engineer's cabin.","2020-03-15","","Completed","2020-02-28","No","No","No","Internal"]
[null,null,null,null,8306,"100_13/12/2019 03:50:55","2019-12-05","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Both life boats lookout glasses dirty/not clear.","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.29","High","","","Glasses cleaned","2020-04-20","","Completed","2020-03-20","No","No","No","Internal"]
[null,null,null,null,8307,"100_13/12/2019 04:01:14","2019-12-05","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Galley exhaust mushrooms on bridge deck wasted on edges/junction box area.","Miscellaneous","Structural Condn. / WT integrity ","Inappropriate Procedure","11.7","High","","","Vent Head taken out, found casing wasted completely from inside. New casing made and fitted back.","2020-02-04","","Completed","2020-01-13","No","No","No","Internal"]
[null,null,null,null,8308,"100_13/12/2019 04:10:04","2019-12-05","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","General service & GMDSS batteries expired & with poor performance","Critical Equip.,Navigation - GMDSS & Communication","Navigation","Equipment Related","4.23","High","","","Replaced with new batteries upon receipt","2020-12-31","","Completed","2020-01-15","No","No","No","Internal"]
[null,null,null,null,8330,"100_17-12-2019 07:24:42","2019-12-05","Defect","Ship Staff","Ship Staff Insp.","Both Lifeboat Batteries both the batteries expired\t","LSA / FFA","Safety / LSA / FFA","Equipment Related","10.36","Very High","","","Replace with new batteires upon receipt","2020-01-31","PROM190005","Completed","2020-01-04","No","No","No","Internal"]
[null,null,null,null,8331,"100_17-12-2019 07:34:00","2019-12-05","Defect","Ship Staff","Ship Staff Insp.","GMDSS Asnd Ship general service Batteries Expired","Critical Equip.","Emgcy. Systems","Equipment Related","4.23","High","","","Renewed with new Batteries.","2020-01-31","PROM190002","Completed","2020-01-15","No","No","No","Internal"]
[null,null,null,null,8332,"100_17-12-2019 07:36:40","2019-12-05","Defect","Ship Staff","Ship Staff Insp.","Fire Alarm Panel Batteries Expired","LSA / FFA","Safety / LSA / FFA","Equipment Related","10.36","Very High","","","Batteries Recieved, and replaced.","2020-03-31","PROM200040","Completed","2020-04-02","No","No","No","Internal"]
[null,null,null,null,8338,"100_19/12/2019 20:38:09","2019-12-05","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Stbd side ship name board light fixture support corroded.","Miscellaneous","General Appearance","Inappropriate Procedure","11.5","Medium","","","Corroded area de-rusted and painting carried out.","2020-08-31","","Completed","2020-04-08","No","No","No","Internal","Revert reason for not completing this job."]
[null,null,null,null,8339,"100_19/12/2019 21:00:19","2019-12-05","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Monorail platform wasted and holed at various locations","Deck - Machinery","General Appearance","Inappropriate Procedure","8.5","Very High","","","Repair work in vessel's scope has been completed.","2020-08-31","","Completed","2020-03-19","Yes","No","No","Internal","Job can be performed in ballast passage with relevant permission from safety department. Let us know vessel intention for same."]
[null,null,null,null,8340,"100_19/12/2019 21:35:20","2019-12-05","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Monorail cable guide rollers frozen","Deck - Machinery","General Appearance","Equipment Related","8.5","Very High","","","Rollers freed up","2020-03-05","","Completed","2020-02-24","No","No","No","Internal"]
[null,null,null,null,8341,"100_19/12/2019 21:40:41","2019-12-05","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Both port & stbd sidelight top plate corroded","Miscellaneous","Navigation","Inappropriate Procedure","4.8","Medium","","","Vessel have completed job in vessel's scope with screw arrangement for corroded sidelight top plate. Permanent repairs to be done in DD. Job included in DD specs. ","2020-08-31","","Completed","2020-02-28","No","No","No","Internal","Job can be performed in ballast passage with relevant permission from safety department. Let us know vessel intention for same."]
[null,null,null,null,8360,"100_13/12/2019 02:00:13","2019-12-05","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Missing handle of hydraulic isolation valve of mooring which forward of deck seal.","Deck - Pipe / Fittings,Deck - Mooring Machinery","Mooring","Equipment Related,Inappropriate Procedure","9.14","Medium","","","Valve handle / wheel replaced","2019-12-15","","Completed","2019-12-06","No","No","No","Internal"]
[null,null,null,null,8368,"100_17-12-2019 07:09:05","2019-12-05","Defect","Ship Staff","Ship Staff Insp.","Pump Room Bilge Alarm indication not showing in CCR","Miscellaneous","Cargo / Ballast Systems","Equipment Related","6.11","High","","","Indication light renewed","2019-12-10","","Completed","2019-12-05","No","No","No","Internal"]
[null,null,null,null,8376,"100_Wed Jun 12 2019 17:53:55 GMT+0000 (Coordinated Universal Time)","2019-12-05","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Both port & stbd side lifeboat canopy light foundation rusted.","LSA / FFA","Safety / LSA / FFA","Equipment Related,External Factors","5.27","Medium","","","To fabricate new light foundation","2020-02-04","","Completed","2019-12-24","No","No","No","Internal"]
[null,null,null,null,8377,"100_Wed Jun 12 2019 17:58:13 GMT+0000 (Coordinated Universal Time)","2019-12-05","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","SIP markings missing on all accommodation vents.","Miscellaneous","Cargo / Ballast Systems","Inappropriate Procedure","11.8","Low","","","All vents SIP Markings done.","2020-01-15","","Completed","2020-01-10","No","No","No","Internal"]
[null,null,null,null,8378,"100_Wed Jun 12 2019 18:03:25 GMT+0000 (Coordinated Universal Time)","2019-12-05","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","IMO posters and symbols on deck faded in various locations","LSA / FFA","Safety / LSA / FFA","Inappropriate Procedure,Knowledge Based","5.27","Medium","","","IMO posters and symbols on deck replaced with new one.","2020-04-15","","Completed","2020-03-30","No","No","No","Internal"]
[null,null,null,null,8379,"100_Fri Jul 12 2019 11:17:30 GMT+0000 (Coordinated Universal Time)","2019-12-05","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Port & Stbd sides liferaft maintenance davits frozen.","LSA / FFA,Miscellaneous","Safety / LSA / FFA","Equipment Related,Inappropriate Procedure","5.28","Very High","","","Davit  freed up","2020-03-04","","Completed","2020-02-21","No","No","No","Internal"]
[null,null,null,null,8380,"100_Fri Jul 12 2019 11:26:18 GMT+0000 (Coordinated Universal Time)","2019-12-05","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Propeller warning boards in poop deck in faded condition","Miscellaneous","General Appearance","Behaviour Based,Inappropriate Procedure","11.3","Medium","","","New markings made.","2020-03-14","","Completed","2020-02-25","No","No","No","Internal"]
[null,null,null,null,null,"100_13/12/2019 02:26:47","2019-12-05","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Wasted forward section of MOT ladder","Miscellaneous","General Appearance","Inappropriate Procedure",5.47,"Medium","Not Applicable","Not Applicable","Temporary repair on wasted forward section of MOT ladder completed. Job has been added in DD specs","2020-09-30",null,"Completed","2020-06-17","No",null,null,"Internal"]
[null,null,null,null,null,"100_13/12/2019 03:24:33","2019-12-05","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Broken tiles, missing mirror cabinets & dirty bulkheads/floors for crew toilets.","Accommodation","MLC Related","External Factors,Inappropriate Procedure",11.13,"Low","Not Applicable","Not Applicable","Broken tiles replaced with new one and dirty bulkheads for crew toilets cleaned","2020-06-30",null,"Completed","2020-06-29","No",null,null,"Internal"]
[null,null,null,null,8294,"100_Fri Jul 12 2019 11:43:39 GMT+0000 (Coordinated Universal Time)","2019-12-06","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Section of tank gauging pipeline support found wasted near 3 across area and line in contact with deck.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related,Inappropriate Procedure","11.4","Very High","","","Pipeline temporary clamping arrangement made with adjacent support brackets.","2019-12-15","","Completed","2020-12-12","No","No","No","Internal"]
[null,null,null,null,8333,"100_17-12-2019 07:39:46","2019-12-07","Other","Ship Staff","Ship Staff Insp.","Service Air/Compressor Out of Use as vessel doesnt have necessary grade of oil.","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Recieved new Oil, Oil replenished and Compressor put in service","2020-03-15","PROM190007","Completed","2020-04-02","No","No","No","Internal"]
[null,null,null,null,8342,"100_19/12/2019 21:44:56","2019-12-07","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Emergency generator filling pipe and vent heavily rusted.","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","Inappropriate Procedure","11.7","High","","","New pipe fabricated for vent head and filling pipe.Fitted and painted","2020-03-06","","Completed","2020-01-13","No","No","No","Internal"]
[null,null,null,null,8343,"100_19/12/2019 23:43:03","2019-12-07","Defect","Ship Staff","Ship Staff Insp.","Basin taps inside Galley and Crew Pantry missing / not working","Accommodation","MLC Related","Equipment Related","11.13","Low","","","Taps repaired.","2020-07-31","","Completed","2020-03-01","No","No","No","Internal"]
[null,null,null,null,8345,"100_20/12/2019 00:09:52","2019-12-07","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Forward embarkation ladder observed to be in poor condition","LSA / FFA","Safety / LSA / FFA","Inappropriate Procedure","5.29","High","","","New Ladder received and replaced.","2020-05-06","","Completed","2020-04-02","No","No","No","Internal"]
[null,null,null,null,8357,"100_20/12/2019 01:24:01","2019-12-07","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Liferafts emergency light box foundation wasted","Deck - Pipe / Fittings","General Appearance","Equipment Related,Inappropriate Procedure","5.28","Very High","","","Light foundation  renewed","2020-04-06","","Completed","2020-03-31","No","No","No","Internal"]
[null,null,null,null,8358,"100_20/12/2019 01:27:38","2019-12-07","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Boss connecting links in poor condition were fitted to few of the wires, while majority of the links are mandal shackles","Miscellaneous","Mooring","Equipment Related","9.12","Medium","","","Mandal shackles in place.","2020-07-31","","Completed","2019-12-31","No","No","No","Internal"]
[null,null,null,null,8367,"100_19/12/2019 13:40:57","2019-12-07","Defect","Ship Staff","Ship Staff Insp.","One no. SCBA face mask neck straps found broken.","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.43","High","","","Strap replaced with spare onboard","2019-12-08","","Completed","2019-12-07","No","No","No","Internal"]
[null,null,null,null,8369,"100_20/12/2019 00:15:47","2019-12-07","Defect","Ship Staff","Ship Staff Insp.","Starboard side anchor not hawsed in completely","Miscellaneous","Mooring","Inappropriate Procedure","9.21","Medium","","","Kink removed from the anchor chain","2020-01-06","","Completed","2019-12-08","No","No","No","Internal"]
[null,null,null,null,8334,"100_19/12/2019 16:13:34","2019-12-08","Defect","Ship Staff","Ship Staff Insp.","Hydraulic leak noticed from No.1 Cargo Pump Discharge  Valve 305 inside pumproom.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","11.4","Very High","","","Leak rectified.","2020-02-08","","Completed","2019-12-22","No","No","No","Internal"]
[null,null,null,null,8347,"100_20/12/2019 00:28:47","2019-12-10","Defect","Ship Staff","Ship Staff Insp.","No.2 stdb and No.5 port WBT level gauges reading erratic.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related,Inappropriate Procedure","8.13","Medium","","","Both 2S and 5P Pneumatic gauge purge pipes found holed. Same repaired and defect rectified. ","2020-03-30","","Completed","2020-01-10","No","No","No","Internal","Vsl was in anchorage drifting from quite some time, kindly update reason for not carrying out fault finding till date."]
[null,null,null,null,8348,"100_20/12/2019 00:37:13","2019-12-10","Defect","Ship Staff","Ship Staff Insp.","Onboard walkie talkies and battery condition is poor","Navigation - GMDSS & Communication","Communication","Equipment Related,Inappropriate Procedure","4.26","Low","","","New walkie talkie and batteries received and put in use.","2020-02-09","","Completed","2020-04-15","No","No","No","Internal"]
[null,null,null,null,8959,"100_24/12/2019 8:54:40 PM","2019-12-11","Breakdown","Ship Staff","Ship Staff Insp.","HFO Purifier # 2 While trying out found in seized condition.\t","E/R - Purifier","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Purifier Major Overhaul carried out. all the bearings o-rings vertical shaft renewed with spare. Condition of all other parts checked. found in good order. Sump Oil Renewed. Purifier tried out.","2019-12-31","","Completed","2019-12-28","No","No","No","Internal"]
[null,null,null,null,8355,"100_20/12/2019 01:14:05","2019-12-12","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Rust weepings observed from anchor wash pipe","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","Equipment Related,Inappropriate Procedure","9.2","Very High","","","Leak rectified.","2020-07-31","","Completed","2020-05-25","No","No","No","Internal"]
[null,null,null,null,8356,"100_20/12/2019 01:20:22","2019-12-12","Defect","Ship Staff","Ship Staff Insp.","Loadicator printer inoperational","Miscellaneous","Cargo / Ballast Systems","Equipment Related","8.4","Medium","","","Spare printer connected to Loadicator.","2020-04-30","","Completed","2020-03-01","No","No","No","Internal"]
[null,null,null,null,8960,"100_25/12/2019 3:13:10 AM","2019-12-16","Defect","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","Latest Company Pilot card ( Company Form 12.01.11.051.01) dated 15 December 2019 did not include minimum steering speed as suggested by BPG 5 Edition annex 3 section A2 Pilot Card.","Navigation - Others","Navigation","Inappropriate Procedure","4.3","Medium","","","Pilot Card revised and put in use","2020-01-15","","Completed","2019-12-17","No","No","No","External"]
[null,null,null,null,8961,"100_25/12/2019 3:46:57 AM","2019-12-16","Defect","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","The vessel was not provided with software ( program) for engine and boiler water as required by Company procedures. Request for the supply was sighted in the onboard record","E/R - Boiler,E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related,External Factors","10.32","Very High","","","Software installed and report generated and send to office for close out.","2020-01-15","","Completed","2019-12-28","No","No","No","External"]
[null,null,null,null,8962,"100_25/12/2019 3:49:30 AM","2019-12-16","Defect","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","SOPEP/VOC/STS Manuals were submitted to Class for Approval. Vessel was waiting\n\nClass approval.","Documentation","Cert. & Docu.","External Factors,Inappropriate Procedure","2.1","Very High","","","Class approval received for the manuals","2020-01-16","","Completed","2019-12-30","No","No","No","External"]
[null,null,null,null,8349,"100_20/12/2019 00:45:12","2019-12-18","Defect","Ship Staff","Ship Staff Insp.","Both AUS vacuum pumps constantly tripping during operation","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.8","Medium","","","AUS to slop NRV valve flap found stuck in open position.Manual valve found seized in closed position.NRV overhauled. Manual valve replaced with pipe section, working satisfactory.","2020-05-17","","Completed","2020-05-07","No","No","No","Internal"]
[null,null,null,null,8351,"100_20/12/2019 00:52:28","2019-12-18","Defect","Ship Staff","Ship Staff Insp.","Slop Stbd valve not holding","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.11","Medium","","","Valve seat ring renewed","2020-02-17","","Completed","2020-01-30","No","No","No","Internal"]
[null,null,null,null,8352,"100_20/12/2019 00:56:54","2019-12-18","Defect","Ship Staff","Ship Staff Insp.","No.1 drop valve observed to be leaking","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.11","Medium","","","Valve seat ring  renewed","2020-02-17","","Completed","2020-02-16","No","No","No","Internal"]
[null,null,null,null,10429,"100_3/2/2020 11:11:41 AM","2019-12-29","Defect","Ship Staff","Ship Staff Insp.","Both Lifeboat Gripes found to be in poor condition.","LSA / FFA","Safety / LSA / FFA","Inappropriate Procedure","5.28","Very High","","","New Lifeboat gripes received and replaced.","2020-02-29","PROM190046","Completed","2020-04-16","No","No","No","Internal"]
[null,null,null,null,10431,"100_5/2/2020 5:53:22 AM","2019-12-29","Defect","Ship Staff","Suptd. Insp.","Vessel is short of one. no.immersion suit required as per safety plan.","LSA / FFA","Safety / LSA / FFA","Human Error,Inappropriate Procedure,Knowledge Based","5.33","High","","","New immersion suit procured and put into missing location.","2020-01-10","","Completed","2020-01-04","No","No","No","Internal"]
[null,null,null,null,10432,"100_3/2/2020 11:49:01 AM","2020-01-01","Defect","Ship Staff","Ship Staff Insp.","Fire hydrant on Poop Deck and Port side upper deck leaking","LSA / FFA","Safety / LSA / FFA","External Factors,Inappropriate Procedure","5.35","Medium","","","Both fire hydrants overhauled and leak rectified","2020-01-09","","Completed","2020-01-02","No","No","No","Internal"]
[null,null,null,null,10433,"100_3/2/2020 11:44:18 AM","2020-01-02","Defect","Ship Staff","Ship Staff Insp.","1S PV Valve leaking from vacuum side","Deck - Pipe / Fittings","Cargo / Ballast Systems","Inappropriate Procedure","8.19","High","","","PV valve overhauled and leak rectified","2020-01-10","","Completed","2020-01-03","No","No","No","Internal"]
[null,null,null,null,10434,"100_5/2/2020 5:16:30 AM","2020-01-07","Defect","Ship Staff","Ship Staff Insp.","Both lifeboat glasses are faded and difficult to view","LSA / FFA","Safety / LSA / FFA","Inappropriate Procedure","5.27","Medium","","","Both lifeboats glasses cleaned & made clear","2020-01-10","","Completed","2020-01-08","No","No","No","Internal"]
[null,null,null,null,null,"100_4/2/2020 2:54:52 AM","2020-01-07","Observation","Ship Staff","Ship Staff Insp.","STBD Side Boat Deck PA System Speaker Not Working.","Miscellaneous","Communication","Equipment Related",5.13,"High","Not Applicable","Not Applicable","Spare Received at Aruba on 15th July 2020. Replaced with new Spare on 16th July 2020","2020-08-31","PROM200010","Completed","2020-07-16","No",null,null,"Internal"]
[null,null,null,null,10435,"100_4/2/2020 2:47:16 AM","2020-01-12","Observation","Ship Staff","Ship Staff Insp.","ME # 4 unit Cooling jacket for cylinder head  leaking o-ring","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","O-Ring and jacket replaced with new spare available onboard while drifting off COLOMBIA awaiting Voyage Instructions.","2020-01-31","","Completed","2020-01-30","No","No","No","Internal"]
[null,null,null,null,12095,"100_3/3/2020 11:46:18 PM","2020-01-13","Defect","Ship Staff","Nav Audit / Verification","Sextant On-board is damaged - Quick Release Clamp and Locking Device is broken and sheared off.","Navigation - Others","Navigation","Equipment Related","4.2","Medium","","","New Sextant received.","2020-04-13","PROM200008","Completed","2020-04-13","No","No","No","Internal"]
[null,null,null,null,10436,"100_5/2/2020 6:07:52 AM","2020-01-28","Defect","Ship Staff","Ship Staff Insp.","One of the CO2 extinguisher hoses was found to be cracked","LSA / FFA","Safety / LSA / FFA","Inappropriate Procedure","5.42","Medium","","","The defective hose was replaced with onboard spare","2020-02-10","","Completed","2020-01-30","No","No","No","Internal"]
[null,null,null,null,12096,"100_9/3/2020 5:26:33 AM","2020-02-06","Defect,Observation","Ship Staff","Ship Staff Insp.","# 1 LT FW Cooler SW Outlet found pin hooled","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Pipe taken out and repairs carried out.Fitted back tried out.","2020-02-07","","Completed","2020-02-07","No","No","No","Internal"]
[null,null,null,null,12097,"100_9/3/2020 5:17:26 AM","2020-02-11","Observation","Ship Staff","Ship Staff Insp.","ME LO cooler SW Outlet pipe Distance pipe found holed.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","REPLACED WITH NEW SPARE DISTANCE PIECE AVAILABLE ONBAORD.","2020-08-28","","Completed","2020-03-13","Yes","No","No","Internal"]
[null,null,null,null,12098,"100_4/4/2020 6:27:19 AM","2020-03-11","Observation","Ship Staff","Ship Staff Insp.","1 P COT PV valve Leaking from Pressure Side\t","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.19","High","","","PV Valve Overhauled.","2020-03-31","","Completed","2020-03-13","No","No","No","Internal"]
[null,null,null,null,null,"100_20/3/2020 4:51:11 AM","2020-03-18","Defect","Ship Staff","Ship Staff Insp.","Light Fitings flanges , bulkhead mounted Outisde accomdation and Deck Found wasted at various location.","Miscellaneous","General Appearance","Equipment Related",11.1,"High","Not Applicable","Not Applicable","Stub pieces cropped and fitted the light flange directy on bulkhead with gasket seal.  ","2020-08-28",null,"Completed","2020-06-19","No",null,null,"Internal"]
[null,null,null,null,12103,"100_4/4/2020 6:45:57 AM","2020-03-19","Defect","Ship Staff","Ship Staff Insp.","Monorial transverse motor Giving Low Insulation Alalrm","Deck - Machinery","Emgcy. Systems","Equipment Related","10.3","Medium","","","MOtor Overhauled.","2020-03-22","","Completed","2020-03-21","No","No","No","Internal"]
[null,null,null,null,12099,"100_4/4/2020 6:37:11 AM","2020-03-28","Observation","Ship Staff","Ship Staff Insp.","Emergency Generator Room Ventialation Fan Mesh Wasted and rusted","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.3","Medium","","","Mesh Renewed And Brackets renewed and desrusted as requied.","2020-04-10","","Completed","2020-04-02","No","No","No","Internal"]
[null,null,null,null,12100,"100_16/5/2020 5:44:21 AM","2020-04-01","Other","Ship Staff","Ship Staff Insp.","ME inlet flowmeter and ME and DG Common Line flowmeter stopped working","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Overhauled  and cleaned internally all parts of both the flowmeters. Working satisfactorily","2020-05-30","","Completed","2020-04-23","No","No","No","Internal"]
[null,null,null,null,12101,"100_30/4/2020 9:29:57 PM","2020-04-14","Observation","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","The ex-proof lifebuoy light, located near cargo tank 5 starboard side was observed at the transparent plastic globe with a crack and moisture inside.","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.31","High","","","Observation was closed out in the course of the inspection. The crew attended and replaced the ex-proof light with a new one of same specification/type.This was verified by the inspector before his departure.","2020-04-30","","Completed","2020-04-14","No","No","No","External"]
[null,null,null,null,12102,"100_16/5/2020 5:34:19 AM","2020-05-08","Observation","Ship Staff","Ship Staff Insp.","ME Tracing Steam line leaking at various places On COPT platform","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Pipe leakage rectified by putting new fittings and tightening fittings as required","2020-05-15","","Completed","2020-05-13","No","No","No","Internal"]
[null,null,null,null,null,"100_3/7/2020 10:44:10 PM","2020-06-01","Defect,Observation","Ship Staff","Ship Staff Insp.","Soot Collecting during routine cosmetic maintenance found plate damage,wasted.Need to crop plates and replace them.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","After Obtaining Hot work Concurrence from office plates sections cropped and replaced with new plates. Cosmectic and corrision portection carried out on the tank.","2020-08-01",null,"Completed","2020-06-20","No",null,null,"Internal"]
[null,null,null,null,null,"100_3/7/2020 11:02:39 PM","2020-06-03","Breakdown","Ship Staff","Ship Staff Insp.","No.2 Steering Gear Motor Magnetic Contactor and 4c Latch Relay Found defective","Miscellaneous","Eng. / Strg. Comp.","Equipment Related",null,null,"Not Applicable","Not Applicable","Same Replaced with new Spare Available onbaord and RO raised for New Spare Contactor and Latch Relay.","2020-06-03","PROM200118","Completed","2020-06-03","No",null,null,"Internal"]
[null,null,null,null,null,"100_16/6/2020 3:19:41 AM","2020-06-08","Observation","Ship Staff","Ship Staff Insp.","Anchor lashing wire for port and stbd anchor found rusted and corroded.","Deck - Mooring Machinery","Mooring","External Factors",9.1999999999999993,"Medium","Not Applicable","Not Applicable","Anchor lashing wire replaced with new one.","2020-06-30",null,"Completed","2020-06-09","No",null,null,"Internal"]
[null,null,null,null,null,"100_19/6/2020 3:58:23 AM","2020-06-10","Observation","Ship Staff","Ship Staff Insp.","1S WBT level gauge showing erratic","Cargo Mach.","Cargo / Ballast Systems","Equipment Related",8.1300000000000008,"Medium","Not Applicable","Not Applicable","Air purge unit for 1S WBT overhauling carried out.Checked for operation,working in good condition.","2020-07-31",null,"Completed","2020-06-17","No",null,null,"Internal"]
[null,null,null,null,null,"100_3/7/2020 10:33:55 PM","2020-06-15","Breakdown,Defect","Ship Staff","Ship Staff Insp.","Emergency Generator Stub Piece for Vent and filling pipe corroded , wasted and pin holed, leading to water contamination of Emergency Genrator Fuel oil tank.","Hull & Tanks","Structural Condn. / WT integrity ","Equipment Related",6.7,"High","Not Applicable","Not Applicable","After Taking Hot Work Permission from office Stub Piece section renewed for both the pipes. FO tank drained cleaned and oil changed.","2020-06-20",null,"Completed","2020-06-17","No",null,null,"Internal"]
[null,null,null,null,null,"100_3/7/2020 10:48:25 PM","2020-06-18","Other","Ship Staff","Ship Staff Insp.","During Routine inspection Funnel Stack Foundation Bolts Found loose.","E/R - Pipes/ valves & fittings","Structural Condn. / WT integrity ","Equipment Related",null,null,"Not Applicable","Not Applicable","All the broken bolts renewed with new spare bolts.","2020-06-21",null,"Completed","2020-06-20","No",null,null,"Internal"]
[null,null,null,null,null,"100_28/6/2020 5:59:12 AM","2020-06-20","Observation","Ship Staff","Ship Staff Insp.","Slop stbd PV valve vacuum side found leaking","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related",8.19,null,"Not Applicable","Not Applicable","Overhauling of Slop stbd PV valve vacuum side carried out.Checked and found working in order.","2020-06-30",null,"Completed","2020-06-23","No",null,null,"Internal"]
[null,null,null,null,null,"100_3/7/2020 10:53:12 PM","2020-06-20","Breakdown","Ship Staff","Ship Staff Insp.","DG # 1 LO Priming Pump motor Trip due overload.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Motor repalced with new spare motor and pump overhauled. RO Raised for New Spare Motor and Pump ","2020-06-21","PROM200130","Completed","2020-06-21","No",null,null,"Internal"]
[null,null,null,null,null,"100_3/7/2020 10:57:42 PM","2020-06-24","Observation","Ship Staff","Ship Staff Insp.","HFO (P) and HFO (S) bunker tanbk forward vent heads distances piece pipe corroded.","Hull & Tanks","Structural Condn. / WT integrity ","Equipment Related",null,null,"Not Applicable","Not Applicable","Pipe sections renewed for both the side.","2020-07-30",null,"Completed","2020-07-16","No",null,null,"Internal"]
[null,null,null,null,null,"100_17/7/2020 5:20:56 AM","2020-07-02","Observation","Ship Staff","Ship Staff Insp.","DG # 1 LO Cooler SW Inlet and Outlet Pipe found Leaking.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related",10.3,null,"Not Applicable","Not Applicable","SW Inlet and Outlet Pipe Renewed with new pipe.","2020-07-05",null,"Completed","2020-07-04","No",null,null,"Internal"]
[null,null,null,null,null,"100_17/7/2020 5:03:33 AM","2020-07-13","Breakdown","Ship Staff","Ship Staff Insp.","Vacuum Condenser Cooling SW Pump Mechanical Seal found leaking","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related",10.3,null,"Not Applicable","Not Applicable","Pump Overhauled. Seal Renewed, shaft heavily eroded same renewed with spare. Motor Overhauled Bearings Renewed","2020-07-15",null,"Completed","2020-07-14","No",null,null,"Internal"]

{"sheet":"Calc","index":2,"n_rows":28,"n_cols":12,"rows_kept":28,"cut":false,"hidden":true,"merged":[]}
["Def_type","Def_cause","Equipments","VIQrefno","Observer_code"]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,"Dim itemSele As Long"]
[null,null,null,null,null,null,null,null,null,null,null,"   dim startRow as integer"]
[null,null,null,null,null,null,null,null,null,null,null,"   startRow=1"]
[null,null,null,null,null,null,null,null,null,null,null,"        For itemSele = 0 To ListBox1.ListCount - 1"]
[null,null,null,null,null,null,null,null,null,null,null,"        If ListBox1.Selected(itemSele) = True Then"]
[null,null,null,null,null,null,null,null,null,null,null,"        Worksheets(\"WorksheetName\").Range(\"A\" & startRow).Value = ListBox1.List(itemSele)"]
[null,null,null,null,null,null,null,null,null,null,null,"        startRow = startRow + 1"]
[null,null,null,null,null,null,null,null,null,null,null,"        End If"]
[null,null,null,null,null,null,null,null,null,null,null,"        Next"]
[null,null,null,null,null,null,null,null,null,null,null,"Dim LastRowA As String"]
[null,null,null,null,null,null,null,null,null,null,null,"        Dim itemSele As Long"]
[null,null,null,null,null,null,null,null,null,null,null,"       Dim startRow as integer"]
[null,null,null,null,null,null,null,null,null,null,null,"        LastRowA = ActiveSheet.Cells(Rows.count, \"A\").End(xlUp).row"]
[null,null,null,null,null,null,null,null,null,null,null,"        startQue = 0"]
[null,null,null,null,null,null,null,null,null,null,null,"        For itemSele = 0 To ListBox1.ListCount - 1"]
[null,null,null,null,null,null,null,null,null,null,null,"        For startRow = 1 To LastRowA"]
[null,null,null,null,null,null,null,null,null,null,null,"        If Worksheets(\"WorksheetName\").Range(\"A\" & startRow).Value = ListBox1.List(itemSele) Then"]
[null,null,null,null,null,null,null,null,null,null,null,"        ListBox1.Selected(itemSele) = True"]
[null,null,null,null,null,null,null,null,null,null,null,"        Exit For"]
[null,null,null,null,null,null,null,null,null,null,null,"        End If"]
[null,null,null,null,null,null,null,null,null,null,null,"        Next j"]
[null,null,null,null,null,null,null,null,null,null,null,"        Next"]
[null,null,null,null,null,null,null,null,null,null,null,"        End If"]

{"sheet":"Areaofobs","index":3,"n_rows":17,"n_cols":2,"rows_kept":17,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Cargo / Ballast Systems",11]
["Cert. & Docu.",2]
["Communication",6]
["Crew Management",3]
["Emgcy. Systems",13]
["Eng. / Strg. Comp.",14]
["General Appearance",15]
["Ice Opns.",17]
["ISM Related",7]
["ISPS Related",10]
["MARPOL Related",9]
["MLC Related",4]
["Mooring",12]
["Navigation",5]
["Safety / LSA / FFA",8]
["Structural Condn. / WT integrity ",16]

{"sheet":"Vessel_type","index":4,"n_rows":1,"n_cols":2,"rows_kept":1,"cut":false,"hidden":true,"merged":[]}
["Vessel_type","ID"]

{"sheet":"Deficiency_type","index":5,"n_rows":8,"n_cols":3,"rows_kept":8,"cut":false,"hidden":true,"merged":[]}
["TITLE","Type of deficiency_description","ID"]
["Breakdown",null,6]
["Critical Equipment",null,4]
["Defect",null,1]
["Guarantee Claim",null,8]
["Non Conformity",null,2]
["Observation",null,3]
["Other",null,7]

{"sheet":"VIQrefno","index":6,"n_rows":427,"n_cols":3,"rows_kept":427,"cut":false,"hidden":true,"merged":[]}
["VIQ_ref_no","Risk Value of observation","ID"]
["1.1","Low",8243]
["1.10","Low",8252]
["1.11","Low",8253]
["1.12","Low",8254]
["1.13","Low",8255]
["1.14","Low",8256]
["1.15","Low",8257]
["1.16","Low",8259]
["1.17","Low",8260]
["1.18","Low",8261]
["1.19","Low",8262]
["1.2","Low",8244]
["1.20","Low",8263]
["1.21","Low",8265]
["1.22","Low",8266]
["1.23","Low",8267]
["1.24","Low",8268]
["1.25","Low",8269]
["1.26","Low",8270]
["1.3","Low",8245]
["1.4","Low",8246]
["1.5","Low",8247]
["1.6","Low",8248]
["1.7","Low",8249]
["1.8","Low",8250]
["1.9","Low",8251]
["1.99","High",11258]
["10.1","Medium",8461]
["10.10","High",8470]
["10.11","Medium",8471]
["10.12","Very High",8472]
["10.13","Very High",8473]
["10.14","Medium",8474]
["10.15","Low",8475]
["10.16","Very High",8476]
["10.17","Very High",8477]
["10.18","High",8478]
["10.19","Very High",8479]
["10.2","Low",8462]
["10.20","High",8480]
["10.21","Medium",8481]
["10.22","Low",8482]
["10.23","Medium",8483]
["10.24","Low",8484]
["10.25","Very High",8485]
["10.26","High",8486]
["10.27","Medium",8487]
["10.28","Low",8488]
["10.29","Medium",8489]
["10.3","Medium",8463]
["10.30","High",8490]
["10.31","Very High",8491]
["10.32","Very High",8492]
["10.33","High",8493]
["10.34","High",8494]
["10.35","Very High",8495]
["10.36","Very High",8496]
["10.37","Medium",8497]
["10.38","Medium",8498]
["10.39","High",8499]
["10.4","High",8464]
["10.40","Medium",8500]
["10.41","Medium",8501]
["10.42","Medium",8502]
["10.43","Medium",8503]
["10.44","Medium",8504]
["10.45","Very High",8505]
["10.46","High",8506]
["10.47","Medium",8507]
["10.48","High",8508]
["10.49","Medium",8509]
["10.5","Low",8465]
["10.50","High",8510]
["10.51","Low",8511]
["10.52","Medium",8512]
["10.53","Medium",8513]
["10.54","High",8514]
["10.55","Low",8515]
["10.6","Very High",8466]
["10.7","Medium",8467]
["10.8","Medium",8468]
["10.9","Medium",8469]
["10.99","High",8516]
["11.1","High",8420]
["11.10","Medium",8429]
["11.11","Very High",8430]
["11.12","Low",8431]
["11.13","Low",8432]
["11.14","Medium",8433]
["11.15","Low",8434]
["11.16","Low",8435]
["11.17","Low",8436]
["11.2","Medium",8421]
["11.3","Medium",8422]
["11.4","Very High",8423]
["11.5","Medium",8424]
["11.6","Medium",8425]
["11.7","High",8426]
["11.8","Low",8427]
["11.9","Low",8428]
["11.99","High",8437]
["12.1","High",8438]
["12.10","High",8448]
["12.11","High",8449]
["12.12","High",8450]
["12.13","High",8451]
["12.14","High",8452]
["12.15","High",8453]
["12.16","High",8454]
["12.17","High",8455]
["12.18","High",8456]
["12.19","High",8457]
["12.2","High",8439]
["12.20","High",8458]
["12.21","High",8459]
["12.3","High",8441]
["12.4","High",8442]
["12.5","High",8443]
["12.6","High",8444]
["12.7","High",8445]
["12.8","High",8446]
["12.9","High",8447]
["12.99","High",8460]
["2.1","Very High",8296]
["2.1.9","Very High",11259]
["2.10","Medium",8304]
["2.11","Medium",8305]
["2.12","Low",8306]
["2.13","Low",8307]
["2.14","Low",8308]
["2.15","Low",8309]
["2.16","Medium",8310]
["2.2","Medium",8297]
["2.3","High",8295]
["2.4","Medium",8298]
["2.5","Medium",8299]
["2.6","Low",8300]
["2.7","High",8301]
["2.8","High",8302]
["2.9","Medium",8303]
["2.99","High",8311]
["3.1","High",8312]
["3.2","Very High",8313]
["3.3","High",8314]
["3.4","Low",8294]
["3.5","Medium",8315]
["3.6","High",8316]
["3.7","Very High",8317]
["3.8","Very High",8318]
["3.99","High",8319]
["4.1","High",8320]
["4.10","High",8329]
["4.11","Medium",8330]
["4.12","Very High",8331]
["4.13","Very High",8332]
["4.14","Very High",8333]
["4.15","Very High",8334]
["4.16","Very High",8335]
["4.17","Very High",8336]
["4.18","Very High",8337]
["4.19","Low",8338]
["4.2","Medium",8321]
["4.20","Very High",8339]
["4.21","High",8340]
["4.22","Low",8341]
["4.23","High",8342]
["4.24","High",8343]
["4.25","Low",8344]
["4.26","Low",8345]
["4.27","High",8346]
["4.3","Medium",8322]
["4.4","High",8323]
["4.5","Very High",8324]
["4.6","Medium",8325]
["4.7","High",8326]
["4.8","Medium",8327]
["4.9","Medium",8328]
["4.99","High",8347]
["5.1","Very High",8517]
["5.10","High",8526]
["5.11","Low",8527]
["5.12","Medium",8528]
["5.13","High",8529]
["5.14","Very High",8530]
["5.15","Medium",8531]
["5.16","Very High",8532]
["5.17","Very High",8533]
["5.18","High",8534]
["5.19","Medium",8535]
["5.2","Very High",8518]
["5.20","Medium",8536]
["5.21","Medium",8537]
["5.22","High",8539]
["5.23","Very High",8540]
["5.24","Very High",8541]
["5.25","Medium",8542]
["5.26","Medium",8543]
["5.27","Medium",8544]
["5.28","Very High",8545]
["5.29","High",8546]
["5.3","Low",8519]
["5.30","High",8547]
["5.31","High",8548]
["5.32","High",8549]
["5.33","High",8550]
["5.34","Low",8551]
["5.35","Medium",8552]
["5.36","Low",8553]
["5.37","Low",8554]
["5.38","High",8555]
["5.39","Very High",8556]
["5.4","High",8520]
["5.40","Very High",8557]
["5.41","Very High",8558]
["5.42","Medium",8559]
["5.43","High",8560]
["5.44","High",8561]
["5.45","Medium",8564]
["5.46","Medium",8565]
["5.47","Medium",8566]
["5.48","Medium",8567]
["5.5","Low",8521]
["5.6","Low",8522]
["5.7","Medium",8523]
["5.8","Medium",8524]
["5.9","Very High",8525]
["5.99","High",8568]
["6.1","Medium",8348]
["6.10","Low",8357]
["6.11","High",8358]
["6.12","Medium",8359]
["6.13","Low",8360]
["6.14","High",8361]
["6.15","High",8362]
["6.16","Very High",8363]
["6.17","Very High",8364]
["6.18","Medium",8365]
["6.19","Low",8366]
["6.2","High",8349]
["6.20","Medium",8367]
["6.21","High",8368]
["6.22","Medium",8369]
["6.3","Low",8350]
["6.4","High",8351]
["6.5","Medium",8352]
["6.6","Medium",8353]
["6.7","High",8354]
["6.8","High",8355]
["6.9","Low",8356]
["6.99","High",8370]
["7.1","High",8371]
["7.10","High",8380]
["7.11","High",8381]
["7.12","High",8382]
["7.13","Medium",8383]
["7.14","Medium",8384]
["7.15","High",8385]
["7.16","High",8386]
["7.17","High",8387]
["7.2","High",8372]
["7.3","Low",8373]
["7.4","Low",8374]
["7.5","Low",8375]
["7.6","Medium",8376]
["7.7","Low",8377]
["7.8","High",8378]
["7.9","High",8379]
["7.99","High",8388]
["8.1","Very High",8569]
["8.10","Very High",8578]
["8.100","Low",11227]
["8.101","Medium",11228]
["8.102","Low",11229]
["8.103","Low",11230]
["8.104","Low",11231]
["8.105","Medium",11232]
["8.106","Medium",11233]
["8.107","Low",11234]
["8.108","High",11235]
["8.109","Very High",11236]
["8.11","Medium",8579]
["8.110","High",11237]
["8.111","Medium",11238]
["8.112","High",11239]
["8.113","Medium",11240]
["8.114","Low",11241]
["8.115","High",11242]
["8.116","Medium",11243]
["8.117","Medium",11244]
["8.118","Medium",11245]
["8.119","High",11246]
["8.12","Medium",8580]
["8.120","High",11247]
["8.121","Medium",11248]
["8.122","High",11249]
["8.123","High",11250]
["8.124","Low",11251]
["8.125","High",11252]
["8.126","Medium",11253]
["8.127","Medium",11254]
["8.13","Medium",8581]
["8.14","Very High",8582]
["8.15","High",8583]
["8.16","Very High",8584]
["8.17","Low",8585]
["8.18","High",8586]
["8.19","High",8587]
["8.199","High",11255]
["8.2","Medium",8570]
["8.20","Medium",8588]
["8.21","High",8589]
["8.22","Very High",8590]
["8.23","Medium",8591]
["8.24","Medium",8592]
["8.25","Very High",8593]
["8.26","High",8594]
["8.27","Medium",8595]
["8.28","Medium",8596]
["8.29","High",8598]
["8.3","Very High",8571]
["8.30","High",8599]
["8.31","High",8600]
["8.32","Low",8601]
["8.33","Medium",8602]
["8.34","High",8603]
["8.35","Medium",8604]
["8.36","Medium",8605]
["8.37","High",8607]
["8.38","Medium",8608]
["8.39","Medium",8609]
["8.4","Medium",8572]
["8.40","High",8610]
["8.41","Medium",8611]
["8.42","Medium",8612]
["8.43","Very High",8613]
["8.44","High",8615]
["8.45","High",8616]
["8.46","Very High",8617]
["8.47","Very High",8618]
["8.48","Medium",8619]
["8.49","High",8620]
["8.5","Very High",8573]
["8.50","Medium",8621]
["8.51","Low",8622]
["8.52","Low",8623]
["8.53","Low",8624]
["8.54","High",8625]
["8.55","Low",11182]
["8.56","Medium",11183]
["8.57","Medium",11184]
["8.58","High",11185]
["8.59","High",11186]
["8.6","Medium",8574]
["8.60","High",11187]
["8.61","Medium",11188]
["8.62","Very High",11189]
["8.63","High",11190]
["8.64","Medium",11191]
["8.65","Low",11192]
["8.66","High",11193]
["8.67","High",11194]
["8.68","High",11195]
["8.69","Medium",11196]
["8.7","High",8575]
["8.70","Medium",11197]
["8.71","Very High",11198]
["8.72","Medium",11199]
["8.73","Medium",11200]
["8.74","High",11201]
["8.75","Medium",11202]
["8.76","Medium",11203]
["8.77","Medium",11204]
["8.78","Medium",11205]
["8.79","Medium",11206]
["8.8","Medium",8576]
["8.80","Medium",11207]
["8.81","Low",11208]
["8.82","Medium",11209]
["8.83","Low",11210]
["8.84","Low",11211]
["8.85","Medium",11212]
["8.86","Medium",11213]
["8.87","Medium",11214]
["8.88","Low",11215]
["8.89","High",11216]
["8.9","High",8577]
["8.90","High",11217]
["8.91","High",11218]
["8.92","Medium",11219]
["8.93","Low",11220]
["8.94","Low",11221]
["8.95","Medium",11222]
["8.96","Medium",11223]
["8.97","Low",11224]
["8.98","High",11225]
["8.99","Medium",11226]
["9.1","Low",8390]
["9.10","Medium",8399]
["9.11","Medium",8400]
["9.12","Medium",8401]
["9.13","Low",8402]
["9.14","Medium",8403]
["9.15","Medium",8404]
["9.16","High",8405]
["9.17","High",8406]
["9.18","Low",8407]
["9.19","Low",8408]
["9.2","Very High",8391]
["9.20","Medium",8409]
["9.21","Medium",8410]
["9.22","Low",8411]
["9.23","Low",8412]
["9.24","Medium",8413]
["9.25","Low",8414]
["9.26","Low",8415]
["9.27","Low",8416]
["9.28","Medium",8417]
["9.29","Low",8418]
["9.3","Very High",8392]
["9.4","High",8393]
["9.5","High",8394]
["9.6","Low",8395]
["9.7","Medium",8396]
["9.8","Medium",8397]
["9.9","Medium",8398]
["9.99","High",8419]

{"sheet":"Equipment_list","index":7,"n_rows":28,"n_cols":3,"rows_kept":28,"cut":false,"hidden":true,"merged":[]}
["TITLE","Equipment_list_description","ID"]
["Accommodation",null,12]
["Cargo Mach.",null,13]
["Critical Equip.",null,16]
["Deck - Machinery",null,18]
["Deck - Mooring Machinery",null,15]
["Deck - Pipe / Fittings",null,20]
["Documentation",null,21]
["E/R - Air Comp.",null,8]
["E/R - Aux. Engine",null,4]
["E/R - Aux. Mach.",null,7]
["E/R - Boiler",null,5]
["E/R - Main Engine",null,3]
["E/R - Pipes/ valves & fittings",null,9]
["E/R - Pumps",null,32]
["E/R - Purifier",null,6]
["Elect. Mach. & Equip.",null,10]
["Hull & Tanks",null,19]
["Inert Gas",null,14]
["LSA / FFA",null,17]
["Miscellaneous",null,22]
["Navigation - DGPS / EPFS / AIS",null,28]
["Navigation - ECDIS",null,25]
["Navigation - Echo Sounder / Speed Log",null,26]
["Navigation - GMDSS & Communication",null,23]
["Navigation - Others",null,11]
["Navigation - RADAR",null,24]
["Navigation - VDR / BNWAS",null,30]

{"sheet":"PSC_MOU","index":8,"n_rows":11,"n_cols":3,"rows_kept":11,"cut":false,"hidden":true,"merged":[]}
["TITLE","PSC_MOU_description","ID"]
["Asia and the Pacific",null,2]
["Caribbean",null,4]
["Europe and the North Atlantic",null,1]
["Latin America",null,3]
["The Black Sea region",null,6]
["The Indian Ocean",null,8]
["The Mediterranean",null,7]
["The Riyadh MoU",null,9]
["USCG",null,10]
["West and Central Africa",null,5]

{"sheet":"Inspection_type","index":9,"n_rows":13,"n_cols":2,"rows_kept":13,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Bunkering Audit",14]
["Cargo Audit",17]
["Engineering Audit",16]
["ISM Audit",2]
["ISPS Audit",3]
["IT Audit",10]
["MLC Audit",1]
["Mooring Audit",9]
["Nav Audit / Verification",8]
["Onboard Training",18]
["Ship Staff Insp.",15]
["Suptd. Insp.",13]

{"sheet":"Deficiency_Cause","index":10,"n_rows":8,"n_cols":3,"rows_kept":8,"cut":false,"hidden":true,"merged":[]}
["TITLE","Deficiency_Cause_description","ID"]
["Behaviour Based",null,1]
["Equipment Related",null,4]
["External Factors",null,5]
["Human Error",null,7]
["Inappropriate Procedure",null,8]
["Industry Issue",null,6]
["Knowledge Based",null,3]

{"sheet":"Observer_code","index":11,"n_rows":3,"n_cols":3,"rows_kept":3,"cut":false,"hidden":true,"merged":[]}
["TITLE","Observer_code_description","ID"]
["Owner / Marine / Tech. Suptd.",null,3]
["Ship Staff",null,2]

{"sheet":"Status_code","index":12,"n_rows":6,"n_cols":3,"rows_kept":6,"cut":false,"hidden":true,"merged":[]}
["TITLE","Status_code_description","ID"]
["Completed",null,6]
["Deferred to D D",null,5]
["In progress",null,3]
["Not Started",null,2]
["Waiting spare",null,4]

{"sheet":"PSC_ref_no","index":13,"n_rows":19,"n_cols":2,"rows_kept":19,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Alarms",9]
["Cargo operations including equipment",7]
["Certificates & Documentation",2]
["Dangerous Goods",13]
["Emergency Systems",5]
["Fire safety",8]
["ISM",16]
["ISPS",17]
["Life saving appliances",12]
["MLC, 2006",18]
["Other",19]
["Pollution Prevention",15]
["Propulsion and auxiliary machinery",14]
["Radio communication",6]
["Safety of Navigation",11]
["Structural condition",3]
["Water/Weathertight condition",4]
["Working and Living Conditions",10]

{"sheet":"Risk_value_of_obs","index":14,"n_rows":1,"n_cols":2,"rows_kept":1,"cut":false,"hidden":true,"merged":[]}
["Risk Value of observation","ID"]

{"sheet":"Year","index":15,"n_rows":18,"n_cols":1,"rows_kept":18,"cut":false,"hidden":true,"merged":[]}
["Year"]
[2014]
[2015]
[2016]
[2017]
[2018]
[2019]
[2020]
[2021]
[2022]
[2023]
[2024]
[2025]
[2026]
[2027]
[2028]
[2029]
[2030]

{"sheet":"Month","index":16,"n_rows":13,"n_cols":1,"rows_kept":13,"cut":false,"hidden":true,"merged":[]}
["Month"]
["Jan"]
["Feb"]
["Mar"]
["Apr"]
["May"]
["Jun"]
["Jul"]
["Aug"]
["Sep"]
["Oct"]
["Nov"]
["Dec"]

{"sheet":"Date_","index":17,"n_rows":32,"n_cols":1,"rows_kept":32,"cut":false,"hidden":true,"merged":[]}
["Date"]
["01"]
["02"]
["03"]
["04"]
["05"]
["06"]
["07"]
["08"]
["09"]
[10]
[11]
[12]
[13]
[14]
[15]
[16]
[17]
[18]
[19]
[20]
[21]
[22]
[23]
[24]
[25]
[26]
[27]
[28]
[29]
[30]
[31]

{"sheet":"Sheet1","index":18,"n_rows":24,"n_cols":6,"rows_kept":24,"cut":false,"hidden":true,"merged":[]}
[]
[null,"ID","E",null,"Date Recorded",1]
[null,"UNIQUE ID","F",null,"Type of Deficiency",2]
[1,"Date Recorded","G",null,"Observer code",3]
["ignore","Vessel Type","H",null,"Type of Inspection",4]
[null,"Internal / External","I",null,"Description of Deficiency",5]
[null,"Drydock","J",null,"Equipment Categories",6]
[null,"Information Sharing","K",null,"Area of Observation",7]
[null,"Critical_item","L",null,"Deficiency Cause",8]
[null,"Deficiency Type","M",null,"VIQ Ref Number",9]
[null,"Deficiency Cause","N",null,"Risk Value of Obs",10]
[null,"Inspection Type","O",null,"PSC Ref Number",11]
[null,"Equipments","P",null,"PSC MOU ID",12]
[null,"VIQ Reference Number","Q",null,"Action Taken or Required",13]
[null,"Risk Value of the observation","R",null,"Target Date",14]
[null,"PSC Reference Number","S",null,"PO Ref No.",15]
[null,"PSC MOU","T",null,"Status Code",16]
[null,"Observer Code","U",null,"Date Completed",17]
[null,"Target Date","V",null,"Drydock",18]
[null,"Status Code","W",null,"Info Sharing",19]
[null,"Description of Deficiency","X",null,"Critical Item Flag",20]
[null,"Action taken / required","Y",null,"Audit Type",21]
[null,"PO ref no","Z"]
[null,"Date completed","AA"]

{"sheet":"Ship_information","index":19,"n_rows":2,"n_cols":3,"rows_kept":2,"cut":false,"hidden":true,"merged":[]}
["Ship_ID","Ship_Name","FILE_NAME"]
["100","PROMOTER (06-06-2020)","100_1591924425385.xlsm"]

{"sheet":"External_Deficiency_type","index":20,"n_rows":5,"n_cols":3,"rows_kept":5,"cut":false,"hidden":true,"merged":[]}
["TITLE","Type of deficiency_description","ID"]
["Condn of Class / Memo",null,5]
["Defect",null,1]
["Non Conformity",null,2]
["Observation",null,3]

{"sheet":"External_Inspection_type","index":21,"n_rows":11,"n_cols":2,"rows_kept":11,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Cargo Audit",17]
["Flag State Insp.",5]
["ISM Audit",2]
["ISPS Audit",3]
["MLC Audit",1]
["Nav Audit / Verification",8]
["OM Insp. (Eg. SIRE / CDI etc.)",6]
["Others (Eg. Insurance etc.)",12]
["PSC Inspection",4]
["Terminal Insp.",11]

{"sheet":"External_Observer_code","index":22,"n_rows":7,"n_cols":3,"rows_kept":7,"cut":false,"hidden":true,"merged":[]}
["TITLE","Observer_code_description","ID"]
["Class Surveyor",null,4]
["FSC Inspector",null,5]
["Others (Eg. Insurance etc.)",null,9]
["PSC Insp.",null,6]
["SIRE / CDI Insp.",null,8]
["Terminal Insp.",null,7]

{"sheet":"Sheet Version","index":23,"n_rows":2,"n_cols":2,"rows_kept":2,"cut":false,"hidden":true,"merged":[]}
["Version","Title"]
["2.0","Version 2.0"]