{"text_format":"1","workbook":"xlsx","n_sheets":24,"sheets":["Mainsheet","Completed","Calc","Areaofobs","Vessel_type","Deficiency_type","VIQrefno","Equipment_list","PSC_MOU","Inspection_type","Deficiency_Cause","Observer_code","Status_code","PSC_ref_no","Risk_value_of_obs","Year","Month","Date_","Sheet1","Ship_information","External_Deficiency_type","External_Inspection_type","External_Observer_code","Sheet Version"],"not_rendered":{"charts":0,"images":5,"macros":1,"external_links":0,"defined_names":12,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Mainsheet","index":0,"n_rows":32,"n_cols":28,"rows_kept":32,"cut":false,"hidden":false,"merged":[[10,8,10,9],[10,12,10,13],[12,6,12,27],[8,6,8,27]]}
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,"Defect - Damage Monitoring Sheet"]
[]
[null,null,null,null,null,null,null,"Date of Report","02-Dec-2020",null,null,"Ship Name","DHT PEONY (24-11-2020)"]
[]
[null,null,null,null,null,null,"VERSION : 2.0"]
[]
[]
[]
[null,null,null,null,"ID","UNIQUE ID","Date Recorded","Type of Deficiency","Observer code","Type of Inspection","Description of Deficiency","Equipment Categories","Area of Observation","Deficiency Cause","VIQ Ref Number","Risk Value of Obs","PSC Ref Number","PSC MOU ID","Action Taken or Required","Target Date","PO Ref No.","Status Code","Date Completed","Drydock","Info Sharing","Critical Item","Audit Type","Superintendent Remarks"]
[null,null,null,null,11904,"50_15/05/2020 5:46:10 PM","2020-04-30","Defect,Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","2C and 4C COT dry check valve cap and handle missing ","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","Equipment Related","","","","","New caps ordered as per DPEO200053. ","2020-12-31","DPEO200053","Waiting spare",null,"No","No","No","Internal"]
[null,null,null,null,13038,"50_07/07/2020 2:15:39 PM","2020-06-15","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","CCR – remote valve indicator- Few not matching with actual open/close Position","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","EO to match by adjusting the potentiometer","2020-12-15","","Not Started",null,"No","No","No","Internal"]
[null,null,null,null,13045,"50_09/07/2020 11:38:23 AM","2020-06-15","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Main deck\tPipe U bolts - Few bolts found rusted ","Deck - Pipe / Fittings","General Appearance","External Factors","","","","","Derusting and painting in progress.","2021-01-15","","In progress",null,"No","No","No","Internal"]
[null,null,null,null,13050,"50_09/07/2020 3:00:50 PM","2020-06-15","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Deck outfittings - At various stages of corrosion ","Deck - Pipe / Fittings","General Appearance","External Factors","","","","","Maintenance in progress","2021-01-15","","In progress",null,"No","No","No","Internal"]
[null,null,null,null,13052,"50_09/07/2020 11:36:22 AM","2020-06-15","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Main Deck - Cable tray running parallel to cargo pipes at various stges of corossion","Deck - Pipe / Fittings","General Appearance","External Factors","","","","","Maintenance in progress","2021-01-15","","In progress",null,"No","No","No","Internal"]
[null,null,null,null,13399,"50_25/07/2020 4:14:22 PM","2020-07-19","Observation","Owner / Marine / Tech. Suptd.","ISM Audit","Numerous used parts from dry dock to be off landed","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","used parts to be shifted on deck and office to be informed regarding the same. Special barge would be required for offlanding so many used items such as valves, pipes etc.","2021-01-10","","Not Started",null,"No","No","No","Internal"]
[null,null,null,null,14213,"50_05/10/2020 5:57:03 PM","2020-09-20","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Mooring winch - Mooring winch foundation rusted ","Deck - Mooring Machinery","Mooring","External Factors","9.15","Medium","","","Maintenance in progress. ","2020-12-15","","In progress",null,"No","No","No","Internal"]
[null,null,null,null,14216,"50_05/10/2020 6:06:07 PM","2020-09-20","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","COW - COW branch line to machines under side rusted – ","Deck - Pipe / Fittings","Cargo / Ballast Systems","External Factors","11.4","Very High","","","Maintenance in progress","2020-12-25","","In progress",null,"No","No","No","Internal"]
[null,null,null,null,14218,"50_05/10/2020 6:00:20 PM","2020-09-20","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Deck pipeline - Main deck pipeline spot rusted","Deck - Pipe / Fittings","Cargo / Ballast Systems","External Factors","11.5","Medium","","","Maintenance in progress","2021-02-20","","In progress",null,"No","No","No","Internal"]
[null,null,null,null,14219,"50_05/10/2020 6:02:25 PM","2020-09-20","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Cargo System - Cargo System hydraulic valve box 2B wasted cover ","Deck - Pipe / Fittings","General Appearance","External Factors","11.3","Medium","","","To renew the wasted part of cover.","2020-12-10","","Not Started",null,"No","No","No","Internal"]
[null,null,null,null,14947,"50_15/11/2020 6:13:18 PM","2020-09-28","Critical Equipment,Defect","Ship Staff","Ship Staff Insp.","SSAS is transmitting actual Security Alert in Test Mode.","Critical Equip.","ISPS Related","Equipment Related","7.7","Low","","","Troubleshooring carried out as instrcted by Mr. kamlesh Solanki. Awaiting further instructions.","2020-12-28","","In progress",null,"No","No","No","Internal"]
[null,null,null,null,null,null,"2020-11-16","Observation","Ship Staff","Ship Staff Insp.","M/E Performance checker DOCTOR unit not operational.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related",null,null,"Not Applicable","Not Applicable","RO raised for 2 new sensors/pickups. Awaiting for spares.","2021-02-16","DPEO200210","Waiting spare",null,"No",null,null,"Internal"]
[null,null,null,null,null,null,"2020-11-16","Non Conformity","Ship Staff","Ship Staff Insp.","Sewage treatment system- discharge rate certificate to be endorsed by ABS class surveyor.","Documentation","Cert. & Docu.","Equipment Related",null,null,"Not Applicable","Not Applicable","During next visit of ABS Class surveyor,we have  plan to get the discharge rate certificate endorsed.","2021-02-16",null,"In progress",null,"No",null,null,"Internal"]
[null,null,null,null,null,null,"2020-11-17","Observation","Ship Staff","Ship Staff Insp.","A/E#3- ADDITIONAL OIL MAX FILTERING UNIT NOT YET INSTALLED.","E/R - Aux. Engine","Eng. / Strg. Comp.","External Factors",null,null,"Not Applicable","Not Applicable","Awaiting for spares of c/case door,FT400 Glacier filter,hoses etc., Oilmax pump with motor already onboard.","2021-02-17","DPEO205109","Waiting spare",null,"No",null,null,"Internal"]
[null,null,null,null,null,null,"2020-11-26","Defect","Ship Staff","Ship Staff Insp.","A/E#3 Unit no.7 suction valve Rocker arm arrangement pushrod bend,need to renew.Also,exh.gas sensor not working.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related",null,null,"Not Applicable","Not Applicable","Awaiting for spares. Also,exh.gas sensor could n't be removed from old cylinder head. no spares onboard.","2020-12-26","DPEO205111. DPEO200187.","Waiting spare",null,"No",null,null,"Internal"]

{"sheet":"Completed","index":1,"n_rows":206,"n_cols":28,"rows_kept":206,"cut":false,"hidden":false,"merged":[[10,8,10,9],[10,12,10,13],[12,6,12,27],[8,6,8,27]]}
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,"Defect - Damage Monitoring Sheet"]
[]
[null,null,null,null,null,null,null,"Date of Report","02-Dec-2020",null,null,"Ship Name","DHT PEONY (24-11-2020)"]
[]
[null,null,null,null,null,null,"VERSION : 2.0"]
[]
[]
[]
[null,null,null,null,"ID","UNIQUE ID","Date Recorded","Type of Deficiency","Observer code","Type of Inspection","Description of Deficiency","Equipment Categories","Area of Observation","Deficiency Cause","VIQ Ref Number","Risk Value of Obs","PSC Ref Number","PSC MOU ID","Action Taken or Required","Target Date","PO Ref No.","Status Code","Date Completed","Drydock","Info Sharing","Critical Item","Audit Type","Superintendent Remarks"]
[null,null,null,null,4087,"50_24/10/2019 3:58:30 PM","2019-01-31","Defect","Ship Staff","Ship Staff Insp.","Pump room overboard ballast line leaking from the flange","Deck - Pipe / Fittings","Cargo / Ballast Systems","Behaviour Based,Equipment Related","","","","","Gasket to be changed during dry dock","2019-10-27","","Completed","2019-10-26","Yes","No","No","Internal"]
[null,null,null,null,4088,"50_24/10/2019 4:20:44 PM","2019-04-12","Defect","Ship Staff","Ship Staff Insp.","DRAFT GAUGE KINE IN 3P WBT HAVE PINHOLE LEAKAGE","Hull & Tanks","Cargo / Ballast Systems","Equipment Related","","","","","COLD REPAIRS DONE, SECTIONS RENEWED IN DRY DOCK","2019-06-30","","Completed","2019-10-26","No","No","No","Internal"]
[null,null,null,null,4089,"50_24/10/2019 4:23:40 PM","2019-04-12","Defect","Ship Staff","Ship Staff Insp.","GAS SAMPLING LINE FOR 3S WBT FWD POINT FOUND FULLY BLOCKED WITH METALLIC OBSTRUCTION IN CENTRELINE BULKHEAD AREA (PASSING FROM 3P TO 3S IN DB)","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","5.21","Medium","","","Line was found to be choked near bulkhead penetration. Same has been cleared during routine tank inspection carried out on 4th April 2020","2021-04-28","","Completed","2020-04-04","Yes","No","No","Internal"]
[null,null,null,null,4090,"50_24/10/2019 4:26:05 PM","2019-04-15","Defect","Ship Staff","Ship Staff Insp.","TG VACUUM CONDENSER SEA WATER INLET VALVE LEAKING FROM BODY.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","TEMPORARY REPAIRS CARRIED OUT/ VALVE RENEWED AFTER RECEIVING SAME.","2019-09-30","DPOE190052","Completed","2019-06-06","No","No","No","Internal"]
[null,null,null,null,4091,"50_24/10/2019 4:28:48 PM","2019-04-15","Defect","Ship Staff","Ship Staff Insp.","ME STARTING AIR PRESSURE ON BRIDGE CONSOLE INCORRECT READING, SHOWS 11 BAR LESS THAN ACTUAL","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","SPARES  RECEIVED  ON 25/05/19","2020-01-15","DPEO190028//RECEIVED ALREADY ON 25/05/19","Completed","2019-05-25","No","No","No","Internal"]
[null,null,null,null,4106,"50_24/10/2019 4:31:30 PM","2019-05-15","Defect","Ship Staff","Ship Staff Insp.","IG BRANCH VALVE FOR 1C,2C,3C,4C,5C,5S,SLOP P&S FOUND LEAKING","Inert Gas","Cargo / Ballast Systems","Equipment Related","","","","","ALL VALVES SEAT RINGS RENEWED","2019-07-30","","Completed","2019-08-28","No","No","No","Internal"]
[null,null,null,null,8079,"50_16/12/2019 11:35:12 AM","2019-05-17","Defect","FSC Inspector","Flag State Insp.","Original contract letters of Fitter, Cook, AB and newly promoted AB was not on board and only scanned copies was on board","Documentation","Crew Management","Inappropriate Procedure","","","","","Original congtract received from manning office","2019-05-25","","Completed","2019-06-27","No","No","No","External"]
[null,null,null,null,4096,"50_24/10/2019 4:44:59 PM","2019-05-18","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","LO PURIFIER #2 STEAM REGULATING VALVE MECHANISM BROKEN AND NOT OPERATIONAL","E/R - Aux. Mach.,E/R - Purifier","Eng. / Strg. Comp.","Equipment Related","","","","","REQUISITION RAISED//RECEIVED,FITTED STILL NOT RERSPONDING, CONVERSATION WITH MAKER ON","2020-01-30","DPEO190154// RECEIVED IN SHIPYARD","Completed","2019-10-23","No","No","No","Internal"]
[null,null,null,null,4101,"50_24/10/2019 4:47:34 PM","2019-05-18","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","FIRE HOSE BOX NEAR LIFEBOAT PORT & STBD FOUNDATION BROKEN\t","LSA / FFA","Eng. / Strg. Comp.","External Factors","","","","","FOUNDATION RENEWED IN DRYDOCK","2019-06-30","","Completed","2019-10-21","No","No","No","Internal"]
[null,null,null,null,4102,"50_24/10/2019 4:57:36 PM","2019-05-18","Defect","Ship Staff","Ship Staff Insp.","2C MAIN VALVE LEAKING CARGO\t\t","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","","","","","SEAT RING RENEWED DURING TANK INSPECTION","2019-08-18","","Completed","2019-09-29","No","No","No","Internal"]
[null,null,null,null,4103,"50_24/10/2019 4:55:14 PM","2019-05-18","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","3S MAIN VALVE SUSPECT LEAKING","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","CHECKED DURING COT INSPECTION , NOT LEAKAGE FOUND","2019-08-18","","Completed","2019-09-29","No","No","No","Internal"]
[null,null,null,null,4086,"50_24/10/2019 4:52:58 PM","2019-05-18","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","GALLEY DISH WASHER NOT OPERATIONAL","Miscellaneous","General Appearance","Equipment Related","","","","","DRAIN TO BE CLEARED IN DD","2019-07-15","","Completed","2019-10-29","No","No","No","Internal"]
[null,null,null,null,4092,"50_24/10/2019 4:33:59 PM","2019-05-18","Defect","Owner / Marine / Tech. Suptd.","Ship Staff Insp.","STROP COUPLING ON ME SCAVANGE RECEIVER DRAIN LINES LEAKING","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","REQUISITION RAISED/ RECEIVED ON 01/10/19 IN DRY DOCK. 7 PIECES RENEWED.","2020-01-16","DPEO190157 // RECEIVED 01/10/19","Completed","2019-12-25","No","No","No","Internal"]
[null,null,null,null,4093,"50_24/10/2019 4:36:27 PM","2019-05-18","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ME NO.1 FUEL PUMP BLOCK SLIGHTLY LEAKING FROM VALVE TOP COVERS","Deck - Machinery,E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","JOB INCLUDED IN REFMAN/// COMPLETED IN DRYDOCK BY SHORE WORKSHOP","2019-10-30","","Completed","2019-10-25","No","No","No","Internal"]
[null,null,null,null,4094,"50_24/10/2019 4:37:55 PM","2019-05-18","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","EGB CLADDING DAMAGED AND TO BE RENEWED","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","JOB INCLUDED IN REFMAN// COMPLETED IN DRYDOCK BY SHORE","2019-08-16","","Completed","2019-10-29","No","No","No","Internal"]
[null,null,null,null,4095,"50_24/10/2019 4:42:44 PM","2019-05-18","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","LO PURIFIER# 1 STEAM REGULATING VALVE MECHANISM BROKEN AND NOT OPERATIONAL","E/R - Boiler,E/R - Purifier","Eng. / Strg. Comp.","Equipment Related","","","","","REQUISISTION RAISED// RECEIVED,FITTED STILL NOT RERSPONDING, CONVERSATION WITH MAKER ON","2020-01-30","DPEO190154// RECEIVED IN SHIPYARD","Completed","2019-10-23","No","No","No","Internal"]
[null,null,null,null,4097,"50_24/10/2019 5:00:07 PM","2019-05-26","Defect","Ship Staff","Ship Staff Insp.","AUX BOILER #2 CHEMICAL DOSING PUMP NOT OPERATIONAL","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","AWAITING SPARES// received, pump renewed","2019-08-20","DPEO190044// received","Completed","2019-11-14","No","No","No","Internal"]
[null,null,null,null,4098,"50_24/10/2019 5:01:43 PM","2019-05-26","Defect","Ship Staff","Ship Staff Insp.","BOILER LOCAL AND MAIN CONTROL PANEL WINDOW AC  NON OPERATIONAL","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","AWAITING SPARES-NA. REPAIRED IN SHIPYARD. AGAIN LOCAL PANEL AC NOT WORKING.","2020-01-20","DPEO190046// RO CANCELLED BY OFFICE","Completed","2019-10-23","No","No","No","Internal"]
[null,null,null,null,8080,"50_16/12/2019 11:37:47 AM","2019-05-26","Non Conformity","Owner / Marine / Tech. Suptd.","ISM Audit","LSA Training manual data not ship specific : Location / Quantity of equipment , Procedure to use the recovery strops/ recover Rescue boat in rough weather missing","LSA / FFA","Safety / LSA / FFA","Human Error","","","","","The Safety and Training manual to be reviewed on a regular basis the by responsible officer","2019-08-26","","Completed","2019-06-15","No","No","No","Internal"]
[null,null,null,null,8081,"50_16/12/2019 11:39:14 AM","2019-05-26","Defect","Owner / Marine / Tech. Suptd.","ISM Audit","Some of the isolation valves in foam room are not marked ","LSA / FFA","Safety / LSA / FFA","Human Error","","","","","The officer and crew were reminded that after any cosmetic maintenance, the markings for identification should be done immediately.\n\nThe safety officer should verify this during his safety rounds.","2019-08-26","","Completed","2019-06-15","No","No","No","Internal"]
[null,null,null,null,8082,"50_16/12/2019 11:41:27 AM","2019-05-26","Defect","Owner / Marine / Tech. Suptd.","ISM Audit","Placard for Garbage in accordance to MARPOL Annex V not available at the Garbage collection/ Handling area ","Documentation","MARPOL Related","Human Error","","","","","The placards were posted in the required locations.","2019-08-26","","Completed","2019-06-15","No","No","No","Internal"]
[null,null,null,null,8083,"50_16/12/2019 11:43:11 AM","2019-05-26","Defect","Owner / Marine / Tech. Suptd.","Mooring Audit","MBL marking not present on the mooring winches (Refer Mooring Equipment Guidelines 4)","Deck - Mooring Machinery","Mooring","Human Error","","","","","Marking were done on the mooring winches","2019-08-26","","Completed","2019-06-15","No","No","No","Internal"]
[null,null,null,null,8084,"50_16/12/2019 11:44:58 AM","2019-05-26","Defect","Owner / Marine / Tech. Suptd.","Nav Audit / Verification","Security levels were not indicated for all legs of the voyage","Navigation - Others","Navigation","Human Error","","","","","The security level included for each leg","2019-08-26","","Completed","2019-06-15","No","No","No","Internal"]
[null,null,null,null,8085,"50_16/12/2019 11:47:11 AM","2019-05-26","Defect","Owner / Marine / Tech. Suptd.","ISM Audit","The log of inspection of lifting equipment in engine room was not upto date. Some of the new chain blocks were not included in the list.","Documentation","Eng. / Strg. Comp.","Human Error","","","","","The list was updated with the new chain blocks also.","2019-08-26","","Completed","2019-06-15","No","No","No","Internal"]
[null,null,null,null,4099,"50_24/10/2019 5:04:39 PM","2019-06-10","Defect","Ship Staff","Ship Staff Insp.","PAINT STORE AND PUMP ROOM STBD SIDE DOOR CHANNEL FOUND IN CORRODED CONDITION","Miscellaneous","Structural Condn. / WT integrity ","Equipment Related","","","","","TO BUILD UP THE HOLES- DOOR REPAIRED AND REFITTED.","2020-03-30","","Completed","2020-01-14","No","No","No","Internal"]
[null,null,null,null,4100,"50_24/10/2019 5:11:40 PM","2019-06-16","Defect","Ship Staff","Ship Staff Insp.","ACCESS HATCH FOR MAST RISER PLATFORM BROKEN FROM HINGES, CHECKERED PLATE THINNED DOWN","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","External Factors","","","","","CHECKERED PLATE CROPPED, NEW PLATE TO BE WELDED AND NEW DOOR TO BE FABRICATED TO BE FITTED","2020-03-30","","Completed","2020-01-02","No","No","No","Internal"]
[null,null,null,null,4105,"50_24/10/2019 5:14:06 PM","2019-06-16","Defect","Ship Staff","Ship Staff Insp.","MAIN MAST PLATFORM ACCESS DOOR HINGES BADLY CORRODED, DOOR UNABLE TO MOVE","Accommodation","General Appearance","External Factors","","","","","DOOR CROPPED AND NEW DOOR FITTED","2019-09-30","","Completed","2019-10-20","No","No","No","Internal"]
[null,null,null,null,4104,"50_24/10/2019 5:18:32 PM","2019-08-20","Defect","Ship Staff","Ship Staff Insp.","BALLAST EDUCTOR SUCTION VALVE BEV 64 SUSPECT LEAKING, TO BE RECTIFIED IN DD","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","","","","","BEV 64 OPENED FOUND PIECE OF RUBBER STUCK AROUND SEAT, SAME REMOVED.SEAT RING FOUND OK","2019-10-15","","Completed","2019-10-22","No","No","No","Internal"]
[null,null,null,null,8086,"50_16/12/2019 11:58:51 AM","2019-09-14","Defect","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","It was observed that several securing screws/bolts were missing from\n\nthe floor plates located in purifier room.","Elect. Mach. & Equip.,E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Human Error","10.29","Medium","","","Missing floor plates screws and bolts fixed","2019-12-14","","Completed","2019-09-14","No","No","No","External"]
[null,null,null,null,8087,"50_16/12/2019 12:02:47 PM","2019-09-14","Defect","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","The paint on midships draft marks, as seen on port side, was noted to\n\nbe faded/removed.\n\nAs per annual survey report issued by Class ABS dated 01 Feb 2019, an outstanding additional\n\nrequirement (No. 32), originally issued in Jan 2018, stated that the 'Loadline marks of the\n\nprevious assigning authority/society in way of the rings are to be grounded off and the 'AB'\n\nmarks are to be permanently marked (punched, welded or raised letters welded to the side\n\nshell) and painted'. Due date: 28 Apr 2021.","Hull & Tanks","Structural Condn. / WT integrity ","Industry Issue","11.2","Medium","","","Completed in dry dock","2021-04-28","","Completed","2019-10-29","No","No","No","External"]
[null,null,null,null,8088,"50_16/12/2019 12:06:48 PM","2019-09-14","Defect","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","The airline section, located near the cargo pump room and connected\n\nto port side pneumatic actuator to operate cargo pump room's vent flap, had been temporarilyrepaired by bandage/putty (length of temporary repair was around 150 mm - pipe size 15A).","Cargo Mach.","Structural Condn. / WT integrity ","Inappropriate Procedure","11.4","Very High","","","New pipe raangement fabricated","2019-12-14","","Completed","2019-10-29","No","No","No","External"]
[null,null,null,null,9053,"50_25/12/2019 3:45:12 PM","2019-11-21","Defect","Ship Staff","Nav Audit / Verification","Some of the entries in deck log book were missing as per the entries to be made bell book/deck log book","Navigation - Others","Navigation","Human Error","","","","","Entries were immediately corrected post audit","2019-12-21","","Completed","2019-11-23","No","No","No","Internal"]
[null,null,null,null,9605,"50_14/01/2020 7:06:42 PM","2019-12-10","Defect","FSC Inspector","OM Insp. (Eg. SIRE / CDI etc.)","LOW INSULATION ON MSB","Elect. Mach. & Equip.","Eng. / Strg. Comp.","External Factors","10.38","Medium","","","INVESTIGATED AND FOUND ONE LIGHT SWITCH ON BRIDGE WINGS WITH MOISTURE FOLLOWING HEAVY RAINS.SAME DISMANTLED AND SERVICED","2020-01-25","","Completed","2019-12-11","No","No","No","External"]
[null,null,null,null,8078,"50_13/12/2019 11:56:45 AM","2019-12-10","Defect","Ship Staff","Ship Staff Insp.","IG SCRUBBER DISCHARGE PIPE HOLED IN MULTIPLE PLACES","Inert Gas","Eng. / Strg. Comp.","Equipment Related","","","","","NO SPARE PIPE ONBOARD, SAME REQUISITIONED and RECEIVED . WILL RENEW IN VOYAGE, ONE LENGTH FABRICATED. BOTH LENGTHS FABRICATED AND FITTED","2020-01-31","DPEO 190265- ALREADY RECEIVED","Completed","2020-01-04","No","No","No","Internal"]
[null,null,null,null,8089,"50_16/12/2019 12:12:03 PM","2019-12-10","Defect","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","Main switch board was noted with an earth alarm on 220 volt panel","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Human Error","10.38","Medium","","","Rectified during inspection.Rectiied during inspection","2019-12-10","","Completed","2019-12-10","No","No","No","External"]
[null,null,null,null,8090,"50_16/12/2019 12:15:44 PM","2019-12-10","Defect","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","The loadlines marked on the vessel refelected a summer deadweight of 299999 MT ( second deepest).The active loadline as per class records was 320013 MT","Hull & Tanks","Structural Condn. / WT integrity ","Knowledge Based","11.2","Medium","","","After further inspection , the correct load lines are found marked on ship side  as per active DWT 299999 MT as per class records ","2020-03-10","","Completed","2020-03-20","No","No","No","External"]
[null,null,null,null,9604,"50_14/01/2020 9:15:43 AM","2020-01-06","Observation","Owner / Marine / Tech. Suptd.,Ship Staff","Suptd. Insp.","CAPACITORS IN FLOURESCENT TO LED LIGHT FITTING CONVERSION IN ACCCOMODATION TO BE DISCONNECTED FROM THE CIRCUIT DURING CONVERSION","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","11.16","Low","","","BEING DONE UPON ANY FITTING CONVERSION ALL FITTINGS IN ACCOMODATION CHECKED. ALL CAPACITORS CONFIRMED DISCONNECTED FOR ALL FLOURESCENT FITTINGS THAT HAVE BEEN REPLACED WITH LED LAMPS","2020-07-05","","Completed","2020-01-28","No","No","No","Internal"]
[null,null,null,null,10569,"50_01/02/2020 11:12:56 AM","2020-01-30","Defect","Ship Staff","Ship Staff Insp.","Wheelhouse Defrosting Heater coil giving 440V low insulation alarm","Navigation - Others","Navigation","Equipment Related","4.7","High","","","New heater coil recvd at singapore. Heater coil fitted and equipment tried out. Working satisfactory","2020-07-30","","Completed","2020-05-18","No","No","No","Internal"]
[null,null,null,null,11898,"50_03/04/2020 7:23:30 AM","2020-02-01","Defect","Ship Staff","Ship Staff Insp.","BEV65 ballast eductor suction valve body cracked and leaking","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","","","","","valve renewed and tried out . Working satisfactory","2020-05-04","DPEO200075","Completed","2020-06-10","No","No","No","Internal",""]
[null,null,null,null,10570,"50_18/02/2020 4:33:28 AM","2020-02-09","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","5P PV Valve mesh corroded and other PV Valve mesh having salt deposits","Inert Gas","Cargo / Ballast Systems","External Factors","8.19","High","","","5P mesh renewed and rest all PV valve mesh cleaned.","2020-05-09","","Completed","2020-02-21","No","No","No","Internal"]
[null,null,null,null,10571,"50_18/02/2020 4:42:41 AM","2020-02-09","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Port and Stbd Anchor wash leaking from the Valve glands.","Deck - Pipe / Fittings","General Appearance","Equipment Related","","","","","Both anchor wash overhauled","2020-05-09","","Completed","2020-03-03","No","No","No","Internal"]
[null,null,null,null,10572,"50_18/02/2020 4:51:17 AM","2020-02-09","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Slop heating coils and COW Branch lines to be De-rusted, buffed and painted","Deck - Pipe / Fittings","General Appearance","Equipment Related","8.15","High","","","Slop heating coils buffed and painted ","2020-05-09","","Completed","2020-02-29","No","No","No","Internal"]
[null,null,null,null,10573,"50_18/02/2020 4:45:24 AM","2020-02-09","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Vapor manifold drains do not have caps at the end.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","","","","","Caps for Vapour manifold Drain pipes - Fabricated and fitted in place","2020-05-09","","Completed","2020-08-19","No","No","No","Internal","Pls land sample at Singapore for fabrication - and update the status of the landed date in DDRL"]
[null,null,null,null,10574,"50_21/02/2020 3:17:16 AM","2020-02-09","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Main Engine Shaft Power Meter not working","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Lemag shaft power sensors received. Sensor renewed.","2020-08-01","DPEO190230","Completed","2020-06-29","No","No","No","Internal"]
[null,null,null,null,10575,"50_18/02/2020 4:29:41 AM","2020-02-09","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Liferaft launching instruction on Port and Stbd accomodation block not fully specific to actual arrangement","LSA / FFA","Safety / LSA / FFA","Behaviour Based,Human Error","5.15","Medium","","","Ship specific life raft launching procedure made and displayed underneath emergency light near liferaft launching station","2020-05-09","","Completed","2020-02-19","No","No","No","Internal"]
[null,null,null,null,10576,"50_18/02/2020 4:11:34 AM","2020-02-09","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Stbd aft vapor manifold drain valve not holding and leaking","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.42","Medium","","","New drain pipe fabricated by hotwork on poop deck.","2020-05-09","","Completed","2020-02-14","No","No","No","Internal"]
[null,null,null,null,10577,"50_18/02/2020 4:21:25 AM","2020-02-09","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","2P and 4S PV Valve vacuum side leaking heavily and other PV Valves need to be checked for Vapour tightness","Inert Gas","Cargo / Ballast Systems","Equipment Related","8.19","High","","","2P and 4S PV valve overhauled.Leak checks carried out for all PV.No leaks observed","2020-05-09","","Completed","2020-02-15","No","No","No","Internal"]
[null,null,null,null,10578,"50_18/02/2020 4:25:13 AM","2020-02-09","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","X Band radar not displaying targets","Navigation - RADAR","Navigation","Equipment Related","","","","","Magnetron replaced and wave guide air blown.X band radar operational.","2020-05-09","","Completed","2020-02-11","No","No","No","Internal"]
[null,null,null,null,10579,"50_18/02/2020 4:49:01 AM","2020-02-09","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Poop deck stbd Mooring winch platform guard dislodged","Deck - Mooring Machinery","Mooring","Human Error","9.14","Medium","","","Platform fixed back by hotwork on poop deck","2020-05-09","","Completed","2020-02-13","No","No","No","Internal"]
[null,null,null,null,10580,"50_18/02/2020 6:18:25 AM","2020-02-09","Observation","Owner / Marine / Tech. Suptd.","Nav Audit / Verification","SAFETY CONTOUR AND SAFTEY DEPTH VALUES WRONGLY CALCULATED IN PASSAGE PLAN FROM JUAYMAH TO PAL.","Navigation - ECDIS","Navigation","Human Error","","","","","SAFETY CONTOUR AND SAFTEY DEPTH VALUES WERE CORRECTED AS PER UKC POLICY","2020-05-08","","Completed","2020-02-10","No","No","No","Internal"]
[null,null,null,null,10581,"50_18/02/2020 6:22:02 AM","2020-02-09","Observation","Owner / Marine / Tech. Suptd.","Nav Audit / Verification","SIMILIAR ENGINE SPEED FOR AHEAD AND ASTERN IS MENTIONED IN THE PILOT CARD","Navigation - Others","Navigation","Human Error","","","","","PILOT CARD WAS CORRECTED FOR ENGINE SPEEDS, AHEAD AND ASTERN VALUES.","2020-05-08","","Completed","2020-02-10","No","No","No","Internal"]
[null,null,null,null,10582,"50_18/02/2020 6:26:34 AM","2020-02-09","Observation","Owner / Marine / Tech. Suptd.","Nav Audit / Verification","BRIDGE COMPUTERS NOT HAVING THE FOLLOWING WARNING POSTERS \" TO USED ONLY FOR WATCH RELATED/NAVIGATION PURPOSES BY WATCHKEEPERS\"","Miscellaneous","Navigation","Inappropriate Procedure","","","","","WARNING POSTER \" TO USED ONLY FOR WATCH RELATED/NAVIGATION PURPOSES BY WATCHKEEPERS\" WERE POSTED ON BRIDGE COMPUTERS.","2020-05-08","","Completed","2020-02-10","No","No","No","Internal"]
[null,null,null,null,10583,"50_18/02/2020 6:40:38 AM","2020-02-09","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","BEST MANAGEMENT PRACTICE POSTER OF \"SWITCH OFF LIGHTS WHEN NOT IN USE\" NOT POSTED IN COMMON SPACES OF ACCOMODATION.","Accommodation","MARPOL Related","Inappropriate Procedure","","","","","BEST MANAGEMENT PRACTICE POSTER OF \"SWITCH OFF LIGHTS WHEN NOT IN USE\" POSTED IN COMMON SPACES OF ACCOMODATION.","2020-05-08","","Completed","2020-02-12","No","No","No","Internal"]
[null,null,null,null,10584,"50_18/02/2020 6:30:53 AM","2020-02-09","Observation","Owner / Marine / Tech. Suptd.","Nav Audit / Verification","MASTER'S NIGHT ORDERS FROM 10TH JAN 2020 TO 31ST JAN 2020 HAVE BEEN WRITTEN FOR 2 DAYS ON A SINGLE PAGE WITH ONLY ONE ACKNOWLEDGEMENT SIGNATURE BY WATCHKEEPERS AT THE END OF THE PAGE.","Miscellaneous","Navigation","Human Error","","","","","WATCHKEEPERS SIGNED NIGHT ORDERS FOR EACH DAY IRRESPECTIVE OF THE PAGE.","2020-05-08","","Completed","2020-02-10","No","No","No","Internal"]
[null,null,null,null,10639,"50_21/02/2020 9:22:10 AM","2020-02-20","Breakdown","Ship Staff","Ship Staff Insp.","2C TGE unit failure","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.19","High","","","2C TGE unit to be replaced","2020-05-20","DPEO200032","Completed","2020-05-04","No","No","No","Internal"]
[null,null,null,null,10640,"50_28/02/2020 8:30:46 PM","2020-02-20","Breakdown","Ship Staff","Ship Staff Insp.","H2S sensor for fixed gas detetion system in pumproom failure","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.46","Very High","","","H2S sensor in Pump room has been replaced with new sensor received in Last call Singapore . Working satisfactory ","2020-05-20","DPEO200035","Completed","2020-07-19","No","No","No","Internal"]
[null,null,null,null,10638,"50_28/02/2020 8:36:34 PM","2020-02-28","Observation","Owner / Marine / Tech. Suptd.","Cargo Audit","Vessel on loaded condition but Pre arrival checks recorded in CCR log on 4th Feb 2020 indicates surface of all WBT`s checked for oil sheen and samples drawn. Pre arrival checks section D item number 15 answered as NA.","Documentation","Cert. & Docu.","Human Error","2.16","Medium","","","Same corrected in checklist and CCR log","2020-05-28","","Completed","2020-03-01","No","No","No","Internal"]
[null,null,null,null,10641,"50_28/02/2020 8:37:51 PM","2020-02-28","Observation","Owner / Marine / Tech. Suptd.","Cargo Audit","Evidence not provided to show that the valve line up was cross checked by two officers. CCR log indicates line up for discharging and venting individually checked by 3 off. ","Documentation","Cargo / Ballast Systems","Human Error","","","","","Same corrected and logged","2020-05-28","","Completed","2020-03-01","No","No","No","Internal"]
[null,null,null,null,10642,"50_28/02/2020 8:39:23 PM","2020-02-28","Observation","Owner / Marine / Tech. Suptd.","Cargo Audit","No evidence to show that entries were made as per 12.21.03.001.00 prior to use of vapour emission control system (oil)","Documentation","Cargo / Ballast Systems","Human Error","","","","","Same logged in CCR log in pre arrival checks","2020-05-28","","Completed","2020-03-01","No","No","No","Internal"]
[null,null,null,null,10643,"50_28/02/2020 8:40:46 PM","2020-02-28","Observation","Owner / Marine / Tech. Suptd.","Cargo Audit","Pre arrival check list was completed after the vessel commenced discharge operation.(07 Feb 2020)  ","Documentation","Cargo / Ballast Systems","Human Error","","","","","corrected for the same ","2020-05-28","","Completed","2020-03-01","No","No","No","Internal"]
[null,null,null,null,10644,"50_29/02/2020 6:17:45 AM","2020-02-28","Observation","Owner / Marine / Tech. Suptd.","Engineering Audit","Serial Number of Purifier and Safety routines (Job Order) of purifiers to be added in PAL PMS","Documentation,E/R - Purifier","Cert. & Docu.","Equipment Related","","","","","CRF FILLED AND SENT TO OFFICE FOR CORRECTION","2020-08-01","","Completed","2020-05-14","No","No","No","Internal"]
[null,null,null,null,10645,"50_28/02/2020 8:42:20 PM","2020-02-28","Observation","Owner / Marine / Tech. Suptd.","Bunkering Audit","Bunkering safety check list 12.04.08.014.00 code A is not signed by both parties.  ","Documentation","Cert. & Docu.","Human Error","","","","","Tick marks were initially placed to record agreement and common signature placed for the column. Now individual places specifiing A have been signed by vessel","2020-05-28","","Completed","2020-02-28","No","No","No","Internal"]
[null,null,null,null,11108,"50_07/03/2020 1:05:05 AM","2020-03-04","Observation","Ship Staff","Ship Staff Insp.","Safety Railing of both hose handling and both provision crane found to be wasted/corroded","Deck - Machinery","Structural Condn. / WT integrity ","Equipment Related","","","","","Wasted sections renewed by hotwork with permission from office","2020-06-04","","Completed","2020-07-24","No","No","No","Internal","Pls include this in REFFMAN, if cannot be repaired and close the defect"]
[null,null,null,null,11107,"50_01/04/2020 2:20:17 AM","2020-03-30","Defect,Observation","Owner / Marine / Tech. Suptd.","Ship Staff Insp.","MS Bolts of hose handling crane working platform to renewed with Stainless steel SUS 316 bolts","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","Equipment Related","","","","","existing bolts were removed from location and checked and were found to be SS . No need for renewal .","2020-06-30","","Completed","2020-05-25","No","No","No","Internal"]
[null,null,null,null,11897,"50_15/05/2020 5:22:54 PM","2020-04-30","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","A deck common toilet door latch spoilt","Accommodation","MLC Related","Equipment Related","","","","","To renew the lock ","2020-07-30","","Completed","2020-06-13","No","No","No","Internal"]
[null,null,null,null,11899,"50_08/05/2020 4:17:56 PM","2020-04-30","Defect,Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Exhasut gas was found leaking from AE#3 Exhasut pipe flange","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Staging made as leaking flange is at a height. Lagging removed and flange bolts to tighened after renewing the gasket","2020-05-28","","Completed","2020-05-20","No","No","No","Internal"]
[null,null,null,null,11900,"50_08/05/2020 4:23:19 PM","2020-04-30","Defect,Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Oil leaking from steering gear system","Critical Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","Minor oil leakage from Ram end part rectified by replacing copper washer at the ram end screw.","2020-10-01","","Completed","2020-09-06","No","No","No","Internal"]
[null,null,null,null,11901,"50_15/05/2020 5:17:57 PM","2020-04-30","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Alleyway floor in front of Ship's Office damaged","Accommodation","General Appearance","Equipment Related","","","","","Deferred to Dry dock","2020-12-30","","Completed","2020-10-31","No","No","No","Internal"]
[null,null,null,null,11902,"50_15/05/2020 5:27:19 PM","2020-04-30","Defect,Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Cargo and Ballast system - Few valve position indicators in CCR not showing correct position of valves. Valve shut but showing open/ partial shut","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","Trouble shooting carried out and rectified valve position.","2020-07-30","","Completed","2020-07-24","No","No","No","Internal"]
[null,null,null,null,11903,"50_15/05/2020 5:31:08 PM","2020-04-30","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","COP Red and Yellow suction pressure gauge not showing zero ","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","Pressure gauge transmitters zero setting done in atmosphere . Found working satisfactory.","2020-07-30","","Completed","2020-06-11","No","No","No","Internal"]
[null,null,null,null,11905,"50_15/05/2020 6:29:04 PM","2020-04-30","Defect,Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Cargo manifold crossover valves reported passing cargo ","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","","","","","Seat rings for all three cross-overs renewed.","2020-07-30","","Completed","2020-06-20","No","No","No","Internal"]
[null,null,null,null,11906,"50_15/05/2020 5:34:33 PM","2020-04-30","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Winches gear oil level not visible as sight glass opaque","Deck - Mooring Machinery","Mooring","Equipment Related","","","","","Main deck is all mooring winches gear oil checked and topped up. Gauge glasses cleaned. Glasses need renewal, no spare on board.","2020-07-30","","Completed","2020-07-10","No","No","No","Internal"]
[null,null,null,null,11907,"50_15/05/2020 5:37:23 PM","2020-04-30","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","PV breaker gauge glass spring loaded shut off valve not operational, Date for last cleaned and inspected not stencilled","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","","","","","Dates to be stencilled , valve to be freed ","2020-07-30","","Completed","2020-05-02","No","No","No","Internal"]
[null,null,null,null,11908,"50_15/05/2020 5:41:35 PM","2020-04-30","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Vapour manifold (P) F drain cock frozen","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","","","","","To free the cock ","2020-07-30","","Completed","2020-05-01","No","No","No","Internal"]
[null,null,null,null,11909,"50_15/05/2020 5:52:41 PM","2020-04-30","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Fire extinguisher in Bosun store last check done in Nov 2019","LSA / FFA","Safety / LSA / FFA","Human Error","","","","","New inspection tag to be attached after proper check of fire extinguisher. All tags to be checked .","2020-05-10","","Completed","2020-05-01","No","No","No","Internal"]
[null,null,null,null,11910,"50_15/05/2020 5:55:56 PM","2020-04-30","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Spare PV valve in midship store (P) not secured","Deck - Pipe / Fittings","Safety / LSA / FFA","Behaviour Based","","","","","To secure the PV valve on the pressure testing kit ","2020-07-30","","Completed","2020-05-01","No","No","No","Internal"]
[null,null,null,null,11911,"50_15/05/2020 6:04:12 PM","2020-04-30","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Chairs from officer's mess room being used in duty mess room ","Accommodation","General Appearance","Human Error","","","","","Chairs to be shifted to Off mess room ","2020-07-30","","Completed","2020-05-03","No","No","No","Internal"]
[null,null,null,null,11912,"50_15/05/2020 6:13:40 PM","2020-04-30","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Anchor chain bitter end (P) hammer missing from location ","Miscellaneous","Safety / LSA / FFA","Human Error","","","","","To put the hammer back and stencil in location - \" DO NOT REMOVE \"","2020-05-10","","Completed","2020-05-02","No","No","No","Internal"]
[null,null,null,null,11913,"50_08/05/2020 4:13:29 PM","2020-04-30","Defect,Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Water was found leaking from EGB into save-all tray","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","EGB isolated. Leaking HP Coil identified and leak rectified","2020-05-28","","Completed","2020-05-15","No","No","No","Internal"]
[null,null,null,null,11914,"50_08/05/2020 4:20:27 PM","2020-04-30","Defect,Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Fuel Oil leaking from AE#2 Fuel pump leak off line","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","All fuel pumps overhauled. no leakage observed","2020-09-28","","Completed","2020-05-16","No","No","No","Internal"]
[null,null,null,null,11915,"50_18/05/2020 3:53:21 PM","2020-05-01","Defect","Ship Staff","Ship Staff Insp.","Incinerator Air damper motor found malfunctioning.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","New motor recvd at singapore. New motor fitted and incinerator operation checked. found satisfactory","2020-06-01","","Completed","2020-05-17","No","No","No","Internal"]
[null,null,null,null,11916,"50_15/05/2020 8:32:53 AM","2020-05-10","Observation","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","Steam leaking from 15k flange of Aux Boiler#1","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Flange bolts to be tightened","2020-05-20","","Completed","2020-05-11","No","No","No","External"]
[null,null,null,null,11917,"50_15/05/2020 6:59:10 PM","2020-05-10","Observation","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","Manifod drip tray drain holes were in poor condition and plugs were unable to firmly fitted. Leaking water at the time of inspection","Deck - Pipe / Fittings","MARPOL Related","Human Error","6.6","Medium","","","Drain holes, cleaned, lubricated, threads redone and fitted in place. Leak tested and found satisfactory.","2020-05-10","","Completed","2020-05-10","No","No","No","External"]
[null,null,null,null,12027,"50_31/05/2020 4:58:59 PM","2020-05-25","Defect","Ship Staff","Ship Staff Insp.","ME FO Booster Pump Discharge pressure guage found to be defective","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Pressure guage replaced with spare one","2020-06-01","","Completed","2020-05-28","No","No","No","Internal"]
[null,null,null,null,12025,"50_31/05/2020 4:57:09 PM","2020-05-27","Defect","Ship Staff","Ship Staff Insp.","ME Unit#6 Exhasut Gas Pyrometer found to be defective","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Exhasut gas pyrometers received.","2020-10-01","DPEO200123","Completed","2020-09-22","No","No","No","Internal"]
[null,null,null,null,12026,"50_31/05/2020 5:04:07 PM","2020-05-30","Breakdown,Defect","Ship Staff","Ship Staff Insp.","FWG High Salinity FW Recirculation solenoid valve found to be defective","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Solenoid valve  replaced with new spare one","2020-07-01","","Completed","2020-05-31","No","No","No","Internal"]
[null,null,null,null,13042,"50_12/06/2020 12:33:20 PM","2020-06-06","Defect,Observation","Ship Staff","Ship Staff Insp.","3P AND 5P BALLAST TANK REMOTE GAUGES NOT SHOWING CORRECT READINGS ","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","Troubleshooting carried out and fault rectified by ETO.","2020-09-02","","Completed","2020-08-22","No","No","No","Internal"]
[null,null,null,null,13029,"50_12/06/2020 10:31:45 AM","2020-06-11","Defect,Observation","Ship Staff","Ship Staff Insp.","Coupling for Emergency hand pump operation for HH crane stbd side found corroded, wasted and holed . Same was leaking oil. ","Deck - Machinery","Cargo / Ballast Systems","Equipment Related","","","","","SPARES RECEIVED AND RENEWED.","2020-09-10","DPEO200124","Completed","2020-08-30","No","No","No","Internal"]
[null,null,null,null,13056,"50_30/06/2020 9:27:03 PM","2020-06-15","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","AC Compressor#1 Condenser SW inlet pressure gauge defective","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","Pressure guage renewed with spare one","2020-06-16","","Completed","2020-06-15","No","No","No","Internal"]
[null,null,null,null,13057,"50_30/06/2020 9:32:01 PM","2020-06-15","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Reefer Compressor#2 belt slipping and making noise","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","Belt renewed with new spare one. Motor distance adjusted.","2020-06-20","","Completed","2020-06-19","No","No","No","Internal"]
[null,null,null,null,13058,"50_30/06/2020 9:44:38 PM","2020-06-15","Defect","Ship Staff","Ship Staff Insp.","Oil leaking from deck air compressor shaft lip seal","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related","","","","","Lip seal renewed with spare one. Compressor boxed back and put in use. No oil leak observed","2020-07-01","","Completed","2020-06-17","No","No","No","Internal"]
[null,null,null,null,13059,"50_05/07/2020 4:13:55 AM","2020-06-15","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Accomm AC Comp- Pressure switch box – cover kept opened and cover lying down\n\n","Miscellaneous","General Appearance","Equipment Related","","","","","switch box covers, panel covers properly fitted back","2020-06-15","","Completed","2020-06-15","No","No","No","Internal"]
[null,null,null,null,13060,"50_05/07/2020 4:16:46 AM","2020-06-15","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","#1 AC Compressor- Save all dirty with oil traces\n\n","Accommodation","General Appearance","Equipment Related","","","","","Save all tray cleaned and painted","2020-06-22","","Completed","2020-06-18","No","No","No","Internal"]
[null,null,null,null,13061,"50_05/07/2020 4:18:55 AM","2020-06-15","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Galley AC unit- Save all dirty – rusty with condesate water collection\n\n","Accommodation","General Appearance","Equipment Related","","","","","Save all tray cleaned and painted","2020-06-22","","Completed","2020-06-19","No","No","No","Internal"]
[null,null,null,null,13062,"50_05/07/2020 4:21:46 AM","2020-06-15","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","AHU room- Natural vent, Louvers frame removed and kept on the floor \n\n","Accommodation","General Appearance","Equipment Related","","","","","Louvre frame installed back","2020-06-15","","Completed","2020-06-15","No","No","No","Internal"]
[null,null,null,null,13063,"50_05/07/2020 4:23:37 AM","2020-06-15","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","#2 AHU\n\nTEV Inspection cover loose and in open condition – securing screws missing\n\n","Accommodation","General Appearance","Equipment Related","","","","","Cover put back with securing screws","2020-06-15","","Completed","2020-06-15","No","No","No","Internal"]
[null,null,null,null,13064,"50_05/07/2020 4:26:45 AM","2020-06-15","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ER Log book\n\nUMS check list complied with comments not mentioned while ER is being changed over to Unmanned\n\n","Documentation","Cert. & Docu.","Human Error","","","","","Comments entered in logbook","2020-06-15","","Completed","2020-06-15","No","No","No","Internal"]
[null,null,null,null,13065,"50_05/07/2020 4:32:40 AM","2020-06-15","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Water Mist System- Valve block, pump casing exterior dirty \n\n","LSA / FFA","General Appearance","Equipment Related","","","","","Motor, pump casing and valve block area cleaned","2020-06-22","","Completed","2020-06-20","No","No","No","Internal"]
[null,null,null,null,13066,"50_05/07/2020 5:00:49 AM","2020-06-15","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","AE 3 -LO leaks observed all over flywheel.\n\n","E/R - Aux. Engine","General Appearance","Inappropriate Procedure","","","","","AE No 3 : Leak rectified and area cleaned","2020-06-22","","Completed","2020-06-20","No","No","No","Internal"]
[null,null,null,null,13067,"50_05/07/2020 5:11:25 AM","2020-06-15","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Aux Boiler : Both boiler remote cables/operating lever for Gauge glass cock valves, safety valves, drain valves – at Boiler base platform (outside ECR) \n\n","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","Aux Boiler : To free the seized wires, operating mechanism and ensure same can be operated remotely\n\n","2020-06-30","","Completed","2020-06-20","No","No","No","Internal"]
[null,null,null,null,13068,"50_05/07/2020 4:28:19 PM","2020-06-15","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","DO tanks- Save all/bulk head near tank drains dirty\n\n","Miscellaneous","General Appearance","Equipment Related","","","","","Save all tray cleaned","2020-06-15","","Completed","2020-06-15","No","No","No","Internal"]
[null,null,null,null,13069,"50_05/07/2020 4:31:04 PM","2020-06-15","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","AE#1,2- Centrufugal filter system found stopped","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","System put back in use","2020-06-15","","Completed","2020-06-15","No","No","No","Internal"]
[null,null,null,null,13070,"50_05/07/2020 4:34:30 PM","2020-06-15","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Vacuum Condensor- Save all stbd side aft area rusty/dirty \n\n","Cargo Mach.","General Appearance","Equipment Related","","","","","Save all tray cleaned","2020-06-21","","Completed","2020-06-19","No","No","No","Internal"]
[null,null,null,null,13071,"50_05/07/2020 4:37:59 PM","2020-06-15","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Tube light Cover- Fitting near LT cooler full of dirt/mud \n\n","Elect. Mach. & Equip.","General Appearance","Equipment Related","","","","","Tube light covers cleaned","2020-06-21","","Completed","2020-06-16","No","No","No","Internal"]
[null,null,null,null,13072,"50_05/07/2020 4:44:29 PM","2020-06-15","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Sea water pumps- Motors, pump exterior dirty\n\n","E/R - Pumps","General Appearance","Equipment Related","","","","","All motor and pump body soap washed","2020-06-30","","Completed","2020-06-24","No","No","No","Internal"]
[null,null,null,null,13073,"50_05/07/2020 4:47:35 PM","2020-06-15","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","HP circulating pump- Signs of water leakage near pump \n\n","E/R - Pumps","General Appearance","Equipment Related","","","","","leak rectified. save all tray cleaned","2020-07-07","","Completed","2020-07-20","No","No","No","Internal"]
[null,null,null,null,13074,"50_05/07/2020 4:53:17 PM","2020-06-15","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ME LO cooler- Area around ME LO cooler, save all dirty\n\n","E/R - Pipes/ valves & fittings","General Appearance","Equipment Related","","","","","Area around ME LO cooler, save all cleaned\n\n","2020-07-15","","Completed","2020-07-02","No","No","No","Internal"]
[null,null,null,null,13075,"50_07/07/2020 2:04:55 PM","2020-06-15","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Gymnasium- Mineral water bottles Stores – blocking space\n\n","Accommodation","General Appearance","Inappropriate Procedure","","","","","Shifted to C-Deck Cable trunk","2020-06-21","","Completed","2020-06-16","No","No","No","Internal"]
[null,null,null,null,13076,"50_07/07/2020 2:21:01 PM","2020-06-15","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Fire control station\tSpare hose kept below QCV operating box/panel, blocking eacy access","LSA / FFA","Safety / LSA / FFA","Human Error","","","","","All spare hoses shifted to safety locker.           Ensured clear/uncluttered access to panels/equipment at FC stationa always","2020-06-15","","Completed","2020-06-15","No","No","No","Internal"]
[null,null,null,null,13077,"50_07/07/2020 2:24:08 PM","2020-06-15","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Fire Man’s Suit - Noticed one suit folded and kept inside the box","LSA / FFA","Safety / LSA / FFA","Human Error","","","","","Suits hung and kept ready to ","2020-06-15","","Completed","2020-06-15","No","No","No","Internal"]
[null,null,null,null,13078,"50_05/07/2020 4:32:44 PM","2020-06-15","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Main engine Governor\n\nActuator exterior, shaft dirty\n\n","E/R - Main Engine","General Appearance","Equipment Related","","","","","Actuator exterior cleaned and greased","2020-06-21","","Completed","2020-06-18","No","No","No","Internal"]
[null,null,null,null,13079,"50_07/07/2020 3:33:38 PM","2020-06-15","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","China passage - Accomm block and Engine casing dirty","Accommodation","General Appearance","External Factors","","","","","oxalic acid wash carried out.","2020-06-15","","Completed","2020-06-24","No","No","No","Internal"]
[null,null,null,null,13080,"50_07/07/2020 5:03:28 PM","2020-06-15","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","EGCS  - Exhaust pipe from funnel to EGCS casing on top deck – insulation cover rusted at both ends","Miscellaneous","General Appearance","Inappropriate Procedure","","","","","Derusted and painted","2020-06-30","","Completed","2020-06-26","No","No","No","Internal"]
[null,null,null,null,13081,"50_07/07/2020 5:10:32 PM","2020-06-15","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ER ventilation fan casing flap - Flaps/frames look rusted ","Miscellaneous","General Appearance","External Factors","","","","","Derusted and painted","2020-08-15","","Completed","2020-06-25","No","No","No","Internal"]
[null,null,null,null,13082,"50_07/07/2020 4:21:23 PM","2020-06-15","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Aft Mooring Winches - Brake band adjusting bolts – clearances hay wire","Deck - Mooring Machinery","Mooring","Equipment Related","","","","","All Aft Winches adjusting bolts replaced with SS and adjusted to 3 MM clearance","2020-07-15","","Completed","2020-07-06","No","No","No","Internal"]
[null,null,null,null,13083,"50_09/07/2020 11:32:23 AM","2020-06-15","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","EGCS/ Scrubber house - All areas/frames, platform dirty – no indication of any one had taken house keeping since last few months!!","Miscellaneous","General Appearance","Human Error","","","","","All areas have been sweeped and mopped. Regular rounds being taken to maintain cleanliness.","2020-07-07","","Completed","2020-06-21","No","No","No","Internal"]
[null,null,null,null,13084,"50_05/07/2020 4:56:40 PM","2020-06-15","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ME Full intermediate shaft rusty ","E/R - Main Engine","General Appearance","Equipment Related","","","","","Shaft cleaned and greased","2020-07-15","","Completed","2020-07-04","No","No","No","Internal"]
[null,null,null,null,13085,"50_09/07/2020 11:48:34 AM","2020-06-15","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Accommodation Gangway - Port side Gangway oil filter, auto drain both rusted and wasted","Deck - Machinery","General Appearance","External Factors","","","","","Renewed Complete Filter Assembly","2020-06-30","","Completed","2020-07-04","No","No","No","Internal"]
[null,null,null,null,13086,"50_09/07/2020 3:10:56 PM","2020-06-15","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Fwd Hyd system tank - Air filter unit fully rusted ","Deck - Mooring Machinery","General Appearance","External Factors","","","","","Air filter unit taken out, maintenance carried out and painted","2020-07-07","","Completed","2020-07-06","No","No","No","Internal"]
[null,null,null,null,13030,"50_30/06/2020 9:36:44 PM","2020-06-15","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Workshop grinding machine imbalanced. ","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","New bearings received. Grinding m/c overhauled,bearings renewed.","2020-07-15","","Completed","2020-09-03","No","No","No","Internal"]
[null,null,null,null,13031,"50_30/06/2020 9:47:38 PM","2020-06-15","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ME Intermediate shaft rusty","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Shaft cleaned/derusted,then light coated with grease.","2020-07-15","","Completed","2020-07-14","No","No","No","Internal"]
[null,null,null,null,13032,"50_30/06/2020 9:51:10 PM","2020-06-15","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Engine room tank top found dirty","Miscellaneous","General Appearance","Equipment Related","","","","","E/R tank top area to be cleaned and painted.","2020-07-15","","Completed","2020-07-22","No","No","No","Internal"]
[null,null,null,null,13033,"50_05/07/2020 4:30:12 AM","2020-06-15","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ME Spare fuel valves- To overhaul,pressure test and keep ready to use.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","ME Spare fuel valves overhauling is in progress. total 15 nos of valves.","2020-09-15","","Completed","2020-11-06","No","No","No","Internal"]
[null,null,null,null,13034,"50_05/07/2020 4:44:55 AM","2020-06-15","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","EGCS sea water chest suction valve remote operating unit, no dates of last tried out .\n\n","Miscellaneous","Cert. & Docu.","Human Error","","","","","EGCS sea water chest suction valve remote operating unit-JOB INCLUDED IN PMS,tred out on 17-July-2020.\n\n\n\n","2020-06-15","","Completed","2020-07-17","No","No","No","Internal"]
[null,null,null,null,13035,"50_05/07/2020 5:05:13 AM","2020-06-15","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","AE #3 : Crank case looks getting pressurized – Sump dip stick missing and kept opened\n\n","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Modified c/case vent line fabricated and fitted.Now,c/case not pressurised.","2020-07-15","","Completed","2020-07-15","No","No","No","Internal"]
[null,null,null,null,13036,"50_05/07/2020 4:58:42 PM","2020-06-15","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Bilge/Tank top found in dirty condition","Miscellaneous","General Appearance","Equipment Related","","","","","tank top cleaned by soap water.","2020-07-15","","Completed","2020-07-07","No","No","No","Internal"]
[null,null,null,null,13037,"50_05/07/2020 5:01:15 PM","2020-06-15","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","AE #1- overhaul/ decarb due.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","A/E#1 DECARB STARTED,JOB IS IN PROGRESS.","2020-10-15","","Completed","2020-11-20","No","No","No","Internal"]
[null,null,null,null,13039,"50_07/07/2020 3:36:37 PM","2020-06-15","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Common deck Store\tWater tight doors, not closing properly","Accommodation","Structural Condn. / WT integrity ","External Factors","","","","","Repaired and proper tightening ensured. Chalk test carried out and found satisfactory. All other WT doors checked and chalk tested.","2020-06-22","","Completed","2020-07-14","No","No","No","Internal"]
[null,null,null,null,13040,"50_07/07/2020 4:14:04 PM","2020-06-15","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Natural vents – covers of various spce at Various stages of corrossion","Accommodation","General Appearance","External Factors","","","","","Spot Derusted and Painted","2020-08-15","","Completed","2020-08-26","No","No","No","Internal"]
[null,null,null,null,13041,"50_07/07/2020 4:16:40 PM","2020-06-15","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Tube light fittings\tFittings on Accommodation front – facing main deck and on other acoomm decks the fitting angle farmes are rusted/corroded","Accommodation","General Appearance","External Factors","","","","","Derusted and painted with 2 coats of primer and finish coat","2020-07-15","","Completed","2020-07-14","No","No","No","Internal"]
[null,null,null,null,13043,"50_07/07/2020 4:18:28 PM","2020-06-15","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Pump room blowers\tBlower Stay pipes/flange ends rusty ","Deck - Pipe / Fittings","General Appearance","External Factors","","","","","Thoroughly derusted and painted with 2 coats of primer and finish coat","2020-07-15","","Completed","2020-07-13","No","No","No","Internal"]
[null,null,null,null,13044,"50_07/07/2020 5:13:06 PM","2020-06-15","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Funnel casing - Dirty/rust weepings","Miscellaneous","General Appearance","External Factors","","","","","Oxalic acid wash followed by high pressure FW wash carried out","2020-08-15","","Completed","2020-07-14","No","No","No","Internal"]
[null,null,null,null,13046,"50_09/07/2020 11:41:22 AM","2020-06-15","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Aft Stern Light - Frame rusted, base corroded","Deck - Pipe / Fittings","General Appearance","External Factors","","","","","Frame derusted and painted.","2020-07-15","","Completed","2020-09-03","No","No","No","Internal"]
[null,null,null,null,13047,"50_09/07/2020 11:43:51 AM","2020-06-15","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Hydraulic remote control valve boxes on deck - Box lips rusted and getting wasted","Deck - Pipe / Fittings","General Appearance","External Factors","","","","","Rusted boxes Derusted and painted. Wasted Sections renewed.","2020-08-15","","Completed","2020-08-19","No","No","No","Internal"]
[null,null,null,null,13048,"50_09/07/2020 11:51:02 AM","2020-06-15","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","PV valves - Few PV valves reported leaking","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","Temporary repair carried out and leaks arrested. Require shore servicing for permanent solution","2020-09-15","","Completed","2020-10-12","No","No","No","Internal"]
[null,null,null,null,13049,"50_09/07/2020 3:03:30 PM","2020-06-15","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Wind Sock - Frame/pipe rusted","Deck - Pipe / Fittings","General Appearance","External Factors","","","","","Derusted and painted with 2 coats of primer and full finish coat","2020-07-15","","Completed","2020-07-13","No","No","No","Internal"]
[null,null,null,null,13051,"50_09/07/2020 3:08:20 PM","2020-06-15","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Fwd Hydraulic system tank - Top area rusted","Deck - Mooring Machinery","General Appearance","External Factors","","","","","Derusted and full coat painted","2020-07-15","","Completed","2020-07-10","No","No","No","Internal"]
[null,null,null,null,13054,"50_30/06/2020 9:20:05 PM","2020-06-15","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Condenser Cooling SW inlet Pressure gauge defective","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Pressure guage renewed with new spare one","2020-06-16","","Completed","2020-06-15","No","No","No","Internal"]
[null,null,null,null,13055,"50_30/06/2020 9:24:25 PM","2020-06-15","Breakdown","Owner / Marine / Tech. Suptd.","Suptd. Insp.","AC Compressor#1 Coupling found broken and compressor could not be used","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","New Coupling received and installed on new AC Compressor. Compressor tried out and put in use","2020-07-01","","Completed","2020-06-25","No","No","No","Internal"]
[null,null,null,null,13087,"50_18/06/2020 9:31:01 AM","2020-06-18","Defect,Observation","Ship Staff","Ship Staff Insp.","Loadicator not going online . Showing error online file expired, not coonected ","Miscellaneous","Cargo / Ballast Systems","Equipment Related","","","","","Rosemount system was restarted 2 times and Loadicator was restarted 2 times . Now the Loadicator is going online except 1P cot ","2020-08-17","","Completed","2020-06-19","No","No","No","Internal"]
[null,null,null,null,13053,"50_23/06/2020 6:25:53 PM","2020-06-23","Observation","Owner / Marine / Tech. Suptd.","Ship Staff Insp.","CCTV cameras not installed in following location :                 1)      2 nos in Bridge (Facing BCC and Radio/Chart tables).\n\n2)      1 no in Cargo control room facing Cargo Console.\n\n3)      2 nos. in ECR (Facing switch board and ECR Console. \n\n4)      1 no. mid section of bridge facing deck area to cover entire deck (if camera is not fitted on bridge wings).\n\n5)      1 no inside scrubber housing (if vessel fitted with scrubber)\n\n","Miscellaneous","ISPS Related","Equipment Related","","","","","CCTV cameras Installed in designated locations and Commissioned.","2020-09-30","","Completed","2020-09-30","No","No","No","Internal"]
[null,null,null,null,13398,"50_31/07/2020 4:30:05 PM","2020-07-17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","At STBD manifold, some bolts were found short.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Industry Issue","","","","","Short Bolts replaced with Longer Bolts","2020-08-20","","Completed","2020-07-20","No","No","No","Internal"]
[null,null,null,null,13400,"50_25/07/2020 4:16:29 PM","2020-07-19","Observation","Owner / Marine / Tech. Suptd.","ISM Audit","At STBD manifold, some bolts were found short. Same to be renewed at the earliest","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","","","","","Short bolts replaced with longer bolts","2020-12-01","","Completed","2020-07-20","No","No","No","Internal"]
[null,null,null,null,13401,"50_25/07/2020 4:18:01 PM","2020-07-19","Observation","Owner / Marine / Tech. Suptd.","ISM Audit","Numerous leak stains found on Main Engine entablature","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Fuel oil leakage from no.2 unit rectified. complete entablature thoroughly cleaned. areas to be painted at the next convenient opportunity.","2020-10-01","","Completed","2020-09-05","No","No","No","Internal"]
[null,null,null,null,13402,"50_25/07/2020 4:21:07 PM","2020-07-19","Defect,Observation","Owner / Marine / Tech. Suptd.","ISM Audit","#2 Main feed Water Pump discharge pressure gauge found defective","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","","","","","discharge pressure guage replaced by new spare.","2020-08-01","","Completed","2020-07-22","No","No","No","Internal"]
[null,null,null,null,13403,"50_25/07/2020 4:33:43 PM","2020-07-19","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Reefer compresoor-Icing observed in suction line","Accommodation","Eng. / Strg. Comp.","Equipment Related","","","","","Filter/drier renewed. Meat room,fish room line filter cleaned. solenoid valve cleaned.","2020-07-29","","Completed","2020-09-03","No","No","No","Internal"]
[null,null,null,null,13404,"50_25/07/2020 4:36:42 PM","2020-07-19","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","#2 AC Compressor-Newly supplied Compressor, reported oil seal leaks","Accommodation","Eng. / Strg. Comp.","Equipment Related","","","","","Mechanical seal flange opened-up,area cleaned thoroughly and fitted back.At present,Negligible leakage only, acceptable.","2020-08-01","","Completed","2020-07-25","No","No","No","Internal"]
[null,null,null,null,13405,"50_25/07/2020 4:38:40 PM","2020-07-19","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","EGG- Exhaust gas leakage from EGB foundation.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","Job created in Refman.Exh.gas leakage from EGB foundation base. To be repaired at Drydock.","2020-09-19","","Completed","2020-11-23","Yes","No","No","Internal"]
[null,null,null,null,13406,"50_25/07/2020 4:40:01 PM","2020-07-19","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","EGB Soot blowers- Soot blower Motor exterior dirty","E/R - Boiler","General Appearance","Equipment Related","","","","","Soot blowers and surrounding area cleaned.","2020-08-01","","Completed","2020-07-22","No","No","No","Internal"]
[null,null,null,null,13407,"50_25/07/2020 4:29:16 PM","2020-07-19","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","LSMGO bunker line valve not gear operated","Deck - Pipe / Fittings","MARPOL Related","Equipment Related","","","","","new gear operated valves received. Butterfly valves replaced by new gear operated valves.","2020-08-04","","Completed","2020-08-14","No","No","No","Internal"]
[null,null,null,null,13408,"50_25/07/2020 4:35:13 PM","2020-07-19","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","#1 AC Compressor-SW line press gauge fitted lose","Accommodation","Eng. / Strg. Comp.","Equipment Related","","","","","New spare pr.gauge with correct size rim, fitted in place and secured.","2020-08-01","","Completed","2020-07-28","No","No","No","Internal"]
[null,null,null,null,13409,"50_25/07/2020 4:42:43 PM","2020-07-19","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ME exh damper- Damper control air line leaks","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Air leakage rectified.","2020-08-01","","Completed","2020-08-07","No","No","No","Internal"]
[null,null,null,null,13410,"50_25/07/2020 4:44:04 PM","2020-07-19","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","EGB- Save alls, adjacent bulkheads, laggings, pipe lines dirty","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","save-alls,adjacent bulkheads.laggings and pipelines cleaned thoroughly, then painted.","2020-09-19","","Completed","2020-09-06","No","No","No","Internal"]
[null,null,null,null,13411,"50_25/07/2020 4:45:18 PM","2020-07-19","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","AE #3- LO leaks from shut down switch","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","A/E#3 SOLEOID VALVE OVERHAULED,O-RINGS RENEWED. LEAKAGE ARRESTED.","2020-08-01","","Completed","2020-08-01","No","No","No","Internal"]
[null,null,null,null,13412,"50_25/07/2020 4:46:50 PM","2020-07-19","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Steam line- 6 Kg service line relief valve leaking","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","safety valve overhauled,pressure tested and put back. leakage stopped.","2020-09-01","","Completed","2020-08-23","No","No","No","Internal"]
[null,null,null,null,13413,"50_25/07/2020 4:48:37 PM","2020-07-19","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Aft Hydraulic system- LO cooler SW pipe flanges leaking ","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Both s.w.inlet & outlet pipes for cooler found leaking, same removed,weld repaired and put back.","2020-08-15","","Completed","2020-08-17","No","No","No","Internal"]
[null,null,null,null,13414,"50_25/07/2020 4:41:10 PM","2020-07-19","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","AE #3- Exhaust gas leaks suspected in the uptakes above EGB platform","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Job created in Refman for d/dock repair.Exhaust gas leakage from A/E#3 uptake-from 2nd dk top,IG platform.staging required for 2nd dk.","2020-09-19","","Completed","2020-11-23","Yes","No","No","Internal"]
[null,null,null,null,13415,"50_25/07/2020 4:50:05 PM","2020-07-19","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Steering room\tPipes on the ceiling, which were opened at DD for EGCS installation – hyd lines, fire line – most of the clamps are not fitted back, vibrations reported","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Hyd.line supports/clamps tightened.","2020-08-01","","Completed","2020-07-27","No","No","No","Internal"]
[null,null,null,null,13416,"50_25/07/2020 4:51:28 PM","2020-07-19","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Incinerator- DO service tank, Quick closing valve leaking","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","Diesel oil leakage rectified.","2020-08-01","","Completed","2020-07-27","No","No","No","Internal"]
[null,null,null,null,13417,"50_25/07/2020 4:56:44 PM","2020-07-19","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Atmos condensor- Sea water leaks from flanges observed","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","atmos.condenser sea water leakage rectified.","2020-08-01","","Completed","2020-08-24","No","No","No","Internal"]
[null,null,null,null,13418,"50_25/07/2020 4:58:06 PM","2020-07-19","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","AE #1- ESM has one alarm lit ","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","In consultation with Technician&Tech.suptd, ESM module renewed. secondary power from Bridge battery charge/discharge panel was off,same put-on. alarm disappeared.","2020-08-01","","Completed","2020-08-08","No","No","No","Internal"]
[null,null,null,null,13419,"50_25/07/2020 4:59:30 PM","2020-07-19","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Main Engine- Old plugged cylinder lubrication holes in the liner has water leakages from few units ","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Water leakage from old plugged cyl.quills rectified.","2020-09-15","","Completed","2020-09-05","No","No","No","Internal"]
[null,null,null,null,13420,"50_25/07/2020 5:02:26 PM","2020-07-19","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Fwd LT cooler Sea water inlet valve leaks fom flange observed\tTo rectify the leaks","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Fwd L.T.Cooler sea water leakage from flange,rectified.","2020-08-19","","Completed","2020-08-24","No","No","No","Internal"]
[null,null,null,null,13421,"50_25/07/2020 5:05:39 PM","2020-07-19","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ME Aft Air cooler- Water washing line, valve leaking","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Leaking valve replaced by spare.","2020-08-01","","Completed","2020-08-07","No","No","No","Internal"]
[null,null,null,null,13422,"50_25/07/2020 4:54:02 PM","2020-07-19","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","EGCS- No spare for air seal motor","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","",""," RO raised for new spare motor.","2020-08-01","","Completed","2020-09-03","No","No","No","Internal"]
[null,null,null,null,13423,"50_25/07/2020 5:12:15 PM","2020-07-19","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Spares Invetory updates- Pending for physical checks and update in PAL","Miscellaneous","Cert. & Docu.","Behaviour Based","","","","","physically checked and updated in PAL PMS.\n\n\n\n","2020-09-19","","Completed","2020-09-06","No","No","No","Internal"]
[null,null,null,null,13424,"50_25/07/2020 5:14:31 PM","2020-07-19","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","LED lights upgrade in ER","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","All tube lights replaced by LED lights. New RO raised for lights and fittings.","2020-08-19","","Completed","2020-09-04","No","No","No","Internal"]
[null,null,null,null,13425,"50_29/07/2020 4:07:46 PM","2020-07-19","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Galley - Dish washer not in use","Accommodation","MLC Related","Equipment Related","","","","","Drain line has been cleared and water supply confirmed.Put in-use.","2020-08-29","","Completed","2020-09-03","No","No","No","Internal"]
[null,null,null,null,13426,"50_25/07/2020 4:55:33 PM","2020-07-19","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Work shop- Welding curtains observed, were of non approved type","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","New welding curtains received from Unitor installed. RO raised for 4 more pcs.","2020-08-01","","Completed","2020-08-26","No","No","No","Internal"]
[null,null,null,null,13427,"50_25/07/2020 5:09:47 PM","2020-07-19","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","EGCS\tEngine load is showing differently on ME remote gauge in ECR and on EGCS panel – 10% more – hence GECS operates on higher load","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","M/E Load transmitter for EGCS has been identified in ECR panel and potentiometer adjusted,so that mainengine stop condition, load shows zero at EGCS.","2020-09-15","","Completed","2020-09-12","No","No","No","Internal"]
[null,null,null,null,13428,"50_25/07/2020 4:10:51 PM","2020-07-19","Observation","Owner / Marine / Tech. Suptd.","ISM Audit","Leak noted at FO Booster Pump pressure switch","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Leak rectified at ME FO Booster pump pressure switch","2020-08-01","","Completed","2020-07-21","No","No","No","Internal"]
[null,null,null,null,13429,"50_25/07/2020 4:25:35 PM","2020-07-19","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Sky light door was kept opened during cargo discharge ops","Miscellaneous","Eng. / Strg. Comp.","Behaviour Based","","","","","sky light door shut immediately","2020-07-19","","Completed","2020-07-19","No","No","No","Internal"]
[null,null,null,null,13430,"50_29/07/2020 4:10:54 PM","2020-07-19","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","SIP natural vents - All natural vents marked as ‘SIP’ were observed in open condition – during cargo disch ops","Accommodation","Safety / LSA / FFA","Human Error","","","","","All SIPs were checked and open ones were shut immediately. Crew briefed regarding same and a practice of checking of the SIPs prior arrival port was put in place","2020-07-19","","Completed","2020-07-19","No","No","No","Internal"]
[null,null,null,null,13431,"50_29/07/2020 4:14:29 PM","2020-07-19","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","COP  - COP #3 leaking from top seal","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","Top seal was slackened and cleaned. Found not leaking. The leak was form the Cooling line connection which was slack due to vibration. Same tightened and clean-up carried out.","2020-07-19","","Completed","2020-07-21","No","No","No","Internal"]
[null,null,null,null,13432,"50_29/07/2020 4:17:53 PM","2020-07-19","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","House keeping - House keeping in public places – Smoke rooms, dining spaces, change rooms, Laundry has scope for improvements","Accommodation","MLC Related","Behaviour Based","","","","","All Public places cleaned, squared-up and orderly arranged.All dustbins emptied on regular basis. Continuous maintenance of cleanliness in progress.","2020-08-02","","Completed","2020-07-25","No","No","No","Internal"]
[null,null,null,null,13433,"50_25/07/2020 4:31:46 PM","2020-07-19","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","COP #3 leaking from top seal","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","top seal flange removed and sea inspected and cleaned. Leak was from cooling line pipe connection. Pipe connection tightened properly","2020-07-26","","Completed","2020-07-22","No","No","No","Internal"]
[null,null,null,null,13856,"50_17/08/2020 3:20:17 PM","2020-08-17","Defect","Ship Staff","Ship Staff Insp.","Personnel Transfer Basket - During 3M inspection, it was observed that one of the strands have broken off from a splice at the bottom frame. Other splices checked and found to be brittle and easily breakable.","Miscellaneous","Safety / LSA / FFA","Equipment Related","","","","","New PTB received while passing Singapore. Old PTB replaced by new one. ","2020-09-30","","Completed","2020-08-25","No","No","No","Internal"]
[null,null,null,null,13857,"50_17/08/2020 3:13:53 PM","2020-08-17","Observation","Ship Staff","Ship Staff Insp.","Lifeboat - Brake release handle eyes for securing remote launching wire shieves found wasted.","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","The brake handles were removed and taken to E/rm workshop. The wasted eyes were cropped and new eyes fabricated and fitted. The handles were brought back and fitted in place.","2020-08-22","","Completed","2020-08-18","No","No","No","Internal"]
[null,null,null,null,14215,"50_29/09/2020 3:48:26 PM","2020-09-10","Defect","Ship Staff","Ship Staff Insp.","Manifold - No 4 Manifold valve Portside observed leaking during discharge operation","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","","","","","Damaged seat ring of the valve renewed.","2020-10-10","","Completed","2020-10-07","No","No","No","Internal"]
[null,null,null,null,14211,"50_05/10/2020 5:49:52 PM","2020-09-20","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Mooring winch -Mooring winch #2 hydraulic oil leakage from inlet line flange ","Deck - Mooring Machinery","Mooring","Equipment Related","11.4","Very High","","","Leakage rectified by replacing O-ring.","2020-10-05","","Completed","2020-11-02","No","No","No","Internal"]
[null,null,null,null,14212,"50_05/10/2020 5:52:35 PM","2020-09-20","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Mooring winch - Mooring winch #3 hydraulic oil leakage from valve block ","Deck - Mooring Machinery","Mooring","Equipment Related","11.4","Very High","","","Leakage rectified by replacing by sealing rings.","2020-10-05","","Completed","2020-11-02","No","No","No","Internal"]
[null,null,null,null,14214,"50_05/10/2020 5:58:41 PM","2020-09-20","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Mooring winch -Mooring winch # 6 brake band rusted - ","Deck - Mooring Machinery","Mooring","External Factors","9.15","Medium","","","Derusted and painted.","2020-10-20","","Completed","2020-10-20","No","No","No","Internal"]
[null,null,null,null,14217,"50_05/10/2020 6:07:52 PM","2020-09-20","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Funnel - Funnel aft side stained ","Miscellaneous","General Appearance","External Factors","11.8","Low","","","Funnel aft side cleaned.","2020-10-15","","Completed","2020-10-08","No","No","No","Internal"]
[null,null,null,null,14220,"50_05/10/2020 6:09:56 PM","2020-09-20","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Hose handling crane - Hose handling crane (STBD) hook noted not free ","Deck - Machinery","Cargo / Ballast Systems","Equipment Related","8.36","Medium","","","Freed up and fresh grease applied","2020-10-05","","Completed","2020-09-30","No","No","No","Internal"]
[null,null,null,null,14221,"50_05/10/2020 5:51:14 PM","2020-09-20","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Mooring winch - Mooring winch #2 hydraulic oil leakage from valve block ","Deck - Mooring Machinery","Mooring","Equipment Related","11.4","Very High","","","Leakage from operating lever rectified.","2020-10-05","","Completed","2020-10-01","No","No","No","Internal"]
[null,null,null,null,14222,"50_05/10/2020 6:04:47 PM","2020-09-20","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","SWL - Lifting lug outside P&S mid ship store SWL not marked ","Miscellaneous","General Appearance","Human Error","11.3","Medium","","","Lug Marked with SWL marking","2020-09-27","","Completed","2020-09-25","No","No","No","Internal"]
[null,null,null,null,14223,"50_05/10/2020 5:55:10 PM","2020-09-20","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Mooring winch - Mooring winch #6 hydraulic oil leakage from valve block ","Deck - Mooring Machinery","Mooring","Equipment Related","11.4","Very High","","","Hyd.oil leakage from operating lever rectified by renewing seal rings.","2020-10-05","","Completed","2020-10-05","No","No","No","Internal"]
[null,null,null,null,14225,"50_29/09/2020 3:56:19 PM","2020-09-21","Defect","Ship Staff","Ship Staff Insp.","1 Sheave Pillar for Stbd gangway swinging wire partially sheared off at base and bent.","Deck - Machinery","Structural Condn. / WT integrity ","Equipment Related","","","","","Temporary repairs and supports fitted by cold work - to carry out permanent repairs at next Dry Dock","2020-09-30","","Completed","2020-09-30","Yes","No","No","Internal"]
[null,null,null,null,14224,"50_03/10/2020 3:04:54 PM","2020-09-30","Defect","Ship Staff","Ship Staff Insp.","During routine inspection it was observed that the Hoisting wire for Port gangway has a lot of Broken strands and needs renewal.","Deck - Machinery","Safety / LSA / FFA","Equipment Related","","","","","Hoisting wire renewed using Spare wire on board.","2020-10-05","","Completed","2020-09-30","No","No","No","Internal"]

{"sheet":"Calc","index":2,"n_rows":28,"n_cols":12,"rows_kept":28,"cut":false,"hidden":true,"merged":[]}
["Def_type","Def_cause","Equipments","VIQrefno","Observer_code"]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,"Dim itemSele As Long"]
[null,null,null,null,null,null,null,null,null,null,null,"   dim startRow as integer"]
[null,null,null,null,null,null,null,null,null,null,null,"   startRow=1"]
[null,null,null,null,null,null,null,null,null,null,null,"        For itemSele = 0 To ListBox1.ListCount - 1"]
[null,null,null,null,null,null,null,null,null,null,null,"        If ListBox1.Selected(itemSele) = True Then"]
[null,null,null,null,null,null,null,null,null,null,null,"        Worksheets(\"WorksheetName\").Range(\"A\" & startRow).Value = ListBox1.List(itemSele)"]
[null,null,null,null,null,null,null,null,null,null,null,"        startRow = startRow + 1"]
[null,null,null,null,null,null,null,null,null,null,null,"        End If"]
[null,null,null,null,null,null,null,null,null,null,null,"        Next"]
[null,null,null,null,null,null,null,null,null,null,null,"Dim LastRowA As String"]
[null,null,null,null,null,null,null,null,null,null,null,"        Dim itemSele As Long"]
[null,null,null,null,null,null,null,null,null,null,null,"       Dim startRow as integer"]
[null,null,null,null,null,null,null,null,null,null,null,"        LastRowA = ActiveSheet.Cells(Rows.count, \"A\").End(xlUp).row"]
[null,null,null,null,null,null,null,null,null,null,null,"        startQue = 0"]
[null,null,null,null,null,null,null,null,null,null,null,"        For itemSele = 0 To ListBox1.ListCount - 1"]
[null,null,null,null,null,null,null,null,null,null,null,"        For startRow = 1 To LastRowA"]
[null,null,null,null,null,null,null,null,null,null,null,"        If Worksheets(\"WorksheetName\").Range(\"A\" & startRow).Value = ListBox1.List(itemSele) Then"]
[null,null,null,null,null,null,null,null,null,null,null,"        ListBox1.Selected(itemSele) = True"]
[null,null,null,null,null,null,null,null,null,null,null,"        Exit For"]
[null,null,null,null,null,null,null,null,null,null,null,"        End If"]
[null,null,null,null,null,null,null,null,null,null,null,"        Next j"]
[null,null,null,null,null,null,null,null,null,null,null,"        Next"]
[null,null,null,null,null,null,null,null,null,null,null,"        End If"]

{"sheet":"Areaofobs","index":3,"n_rows":17,"n_cols":2,"rows_kept":17,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Cargo / Ballast Systems",11]
["Cert. & Docu.",2]
["Communication",6]
["Crew Management",3]
["Emgcy. Systems",13]
["Eng. / Strg. Comp.",14]
["General Appearance",15]
["Ice Opns.",17]
["ISM Related",7]
["ISPS Related",10]
["MARPOL Related",9]
["MLC Related",4]
["Mooring",12]
["Navigation",5]
["Safety / LSA / FFA",8]
["Structural Condn. / WT integrity ",16]

{"sheet":"Vessel_type","index":4,"n_rows":1,"n_cols":2,"rows_kept":1,"cut":false,"hidden":true,"merged":[]}
["Vessel_type","ID"]

{"sheet":"Deficiency_type","index":5,"n_rows":8,"n_cols":3,"rows_kept":8,"cut":false,"hidden":true,"merged":[]}
["TITLE","Type of deficiency_description","ID"]
["Breakdown",null,6]
["Critical Equipment",null,4]
["Defect",null,1]
["Guarantee Claim",null,8]
["Non Conformity",null,2]
["Observation",null,3]
["Other",null,7]

{"sheet":"VIQrefno","index":6,"n_rows":427,"n_cols":3,"rows_kept":427,"cut":false,"hidden":true,"merged":[]}
["VIQ_ref_no","Risk Value of observation","ID"]
["1.1","Low",8243]
["1.10","Low",8252]
["1.11","Low",8253]
["1.12","Low",8254]
["1.13","Low",8255]
["1.14","Low",8256]
["1.15","Low",8257]
["1.16","Low",8259]
["1.17","Low",8260]
["1.18","Low",8261]
["1.19","Low",8262]
["1.2","Low",8244]
["1.20","Low",8263]
["1.21","Low",8265]
["1.22","Low",8266]
["1.23","Low",8267]
["1.24","Low",8268]
["1.25","Low",8269]
["1.26","Low",8270]
["1.3","Low",8245]
["1.4","Low",8246]
["1.5","Low",8247]
["1.6","Low",8248]
["1.7","Low",8249]
["1.8","Low",8250]
["1.9","Low",8251]
["1.99","High",11258]
["10.1","Medium",8461]
["10.10","High",8470]
["10.11","Medium",8471]
["10.12","Very High",8472]
["10.13","Very High",8473]
["10.14","Medium",8474]
["10.15","Low",8475]
["10.16","Very High",8476]
["10.17","Very High",8477]
["10.18","High",8478]
["10.19","Very High",8479]
["10.2","Low",8462]
["10.20","High",8480]
["10.21","Medium",8481]
["10.22","Low",8482]
["10.23","Medium",8483]
["10.24","Low",8484]
["10.25","Very High",8485]
["10.26","High",8486]
["10.27","Medium",8487]
["10.28","Low",8488]
["10.29","Medium",8489]
["10.3","Medium",8463]
["10.30","High",8490]
["10.31","Very High",8491]
["10.32","Very High",8492]
["10.33","High",8493]
["10.34","High",8494]
["10.35","Very High",8495]
["10.36","Very High",8496]
["10.37","Medium",8497]
["10.38","Medium",8498]
["10.39","High",8499]
["10.4","High",8464]
["10.40","Medium",8500]
["10.41","Medium",8501]
["10.42","Medium",8502]
["10.43","Medium",8503]
["10.44","Medium",8504]
["10.45","Very High",8505]
["10.46","High",8506]
["10.47","Medium",8507]
["10.48","High",8508]
["10.49","Medium",8509]
["10.5","Low",8465]
["10.50","High",8510]
["10.51","Low",8511]
["10.52","Medium",8512]
["10.53","Medium",8513]
["10.54","High",8514]
["10.55","Low",8515]
["10.6","Very High",8466]
["10.7","Medium",8467]
["10.8","Medium",8468]
["10.9","Medium",8469]
["10.99","High",8516]
["11.1","High",8420]
["11.10","Medium",8429]
["11.11","Very High",8430]
["11.12","Low",8431]
["11.13","Low",8432]
["11.14","Medium",8433]
["11.15","Low",8434]
["11.16","Low",8435]
["11.17","Low",8436]
["11.2","Medium",8421]
["11.3","Medium",8422]
["11.4","Very High",8423]
["11.5","Medium",8424]
["11.6","Medium",8425]
["11.7","High",8426]
["11.8","Low",8427]
["11.9","Low",8428]
["11.99","High",8437]
["12.1","High",8438]
["12.10","High",8448]
["12.11","High",8449]
["12.12","High",8450]
["12.13","High",8451]
["12.14","High",8452]
["12.15","High",8453]
["12.16","High",8454]
["12.17","High",8455]
["12.18","High",8456]
["12.19","High",8457]
["12.2","High",8439]
["12.20","High",8458]
["12.21","High",8459]
["12.3","High",8441]
["12.4","High",8442]
["12.5","High",8443]
["12.6","High",8444]
["12.7","High",8445]
["12.8","High",8446]
["12.9","High",8447]
["12.99","High",8460]
["2.1","Very High",8296]
["2.1.9","Very High",11259]
["2.10","Medium",8304]
["2.11","Medium",8305]
["2.12","Low",8306]
["2.13","Low",8307]
["2.14","Low",8308]
["2.15","Low",8309]
["2.16","Medium",8310]
["2.2","Medium",8297]
["2.3","High",8295]
["2.4","Medium",8298]
["2.5","Medium",8299]
["2.6","Low",8300]
["2.7","High",8301]
["2.8","High",8302]
["2.9","Medium",8303]
["2.99","High",8311]
["3.1","High",8312]
["3.2","Very High",8313]
["3.3","High",8314]
["3.4","Low",8294]
["3.5","Medium",8315]
["3.6","High",8316]
["3.7","Very High",8317]
["3.8","Very High",8318]
["3.99","High",8319]
["4.1","High",8320]
["4.10","High",8329]
["4.11","Medium",8330]
["4.12","Very High",8331]
["4.13","Very High",8332]
["4.14","Very High",8333]
["4.15","Very High",8334]
["4.16","Very High",8335]
["4.17","Very High",8336]
["4.18","Very High",8337]
["4.19","Low",8338]
["4.2","Medium",8321]
["4.20","Very High",8339]
["4.21","High",8340]
["4.22","Low",8341]
["4.23","High",8342]
["4.24","High",8343]
["4.25","Low",8344]
["4.26","Low",8345]
["4.27","High",8346]
["4.3","Medium",8322]
["4.4","High",8323]
["4.5","Very High",8324]
["4.6","Medium",8325]
["4.7","High",8326]
["4.8","Medium",8327]
["4.9","Medium",8328]
["4.99","High",8347]
["5.1","Very High",8517]
["5.10","High",8526]
["5.11","Low",8527]
["5.12","Medium",8528]
["5.13","High",8529]
["5.14","Very High",8530]
["5.15","Medium",8531]
["5.16","Very High",8532]
["5.17","Very High",8533]
["5.18","High",8534]
["5.19","Medium",8535]
["5.2","Very High",8518]
["5.20","Medium",8536]
["5.21","Medium",8537]
["5.22","High",8539]
["5.23","Very High",8540]
["5.24","Very High",8541]
["5.25","Medium",8542]
["5.26","Medium",8543]
["5.27","Medium",8544]
["5.28","Very High",8545]
["5.29","High",8546]
["5.3","Low",8519]
["5.30","High",8547]
["5.31","High",8548]
["5.32","High",8549]
["5.33","High",8550]
["5.34","Low",8551]
["5.35","Medium",8552]
["5.36","Low",8553]
["5.37","Low",8554]
["5.38","High",8555]
["5.39","Very High",8556]
["5.4","High",8520]
["5.40","Very High",8557]
["5.41","Very High",8558]
["5.42","Medium",8559]
["5.43","High",8560]
["5.44","High",8561]
["5.45","Medium",8564]
["5.46","Medium",8565]
["5.47","Medium",8566]
["5.48","Medium",8567]
["5.5","Low",8521]
["5.6","Low",8522]
["5.7","Medium",8523]
["5.8","Medium",8524]
["5.9","Very High",8525]
["5.99","High",8568]
["6.1","Medium",8348]
["6.10","Low",8357]
["6.11","High",8358]
["6.12","Medium",8359]
["6.13","Low",8360]
["6.14","High",8361]
["6.15","High",8362]
["6.16","Very High",8363]
["6.17","Very High",8364]
["6.18","Medium",8365]
["6.19","Low",8366]
["6.2","High",8349]
["6.20","Medium",8367]
["6.21","High",8368]
["6.22","Medium",8369]
["6.3","Low",8350]
["6.4","High",8351]
["6.5","Medium",8352]
["6.6","Medium",8353]
["6.7","High",8354]
["6.8","High",8355]
["6.9","Low",8356]
["6.99","High",8370]
["7.1","High",8371]
["7.10","High",8380]
["7.11","High",8381]
["7.12","High",8382]
["7.13","Medium",8383]
["7.14","Medium",8384]
["7.15","High",8385]
["7.16","High",8386]
["7.17","High",8387]
["7.2","High",8372]
["7.3","Low",8373]
["7.4","Low",8374]
["7.5","Low",8375]
["7.6","Medium",8376]
["7.7","Low",8377]
["7.8","High",8378]
["7.9","High",8379]
["7.99","High",8388]
["8.1","Very High",8569]
["8.10","Very High",8578]
["8.100","Low",11227]
["8.101","Medium",11228]
["8.102","Low",11229]
["8.103","Low",11230]
["8.104","Low",11231]
["8.105","Medium",11232]
["8.106","Medium",11233]
["8.107","Low",11234]
["8.108","High",11235]
["8.109","Very High",11236]
["8.11","Medium",8579]
["8.110","High",11237]
["8.111","Medium",11238]
["8.112","High",11239]
["8.113","Medium",11240]
["8.114","Low",11241]
["8.115","High",11242]
["8.116","Medium",11243]
["8.117","Medium",11244]
["8.118","Medium",11245]
["8.119","High",11246]
["8.12","Medium",8580]
["8.120","High",11247]
["8.121","Medium",11248]
["8.122","High",11249]
["8.123","High",11250]
["8.124","Low",11251]
["8.125","High",11252]
["8.126","Medium",11253]
["8.127","Medium",11254]
["8.13","Medium",8581]
["8.14","Very High",8582]
["8.15","High",8583]
["8.16","Very High",8584]
["8.17","Low",8585]
["8.18","High",8586]
["8.19","High",8587]
["8.199","High",11255]
["8.2","Medium",8570]
["8.20","Medium",8588]
["8.21","High",8589]
["8.22","Very High",8590]
["8.23","Medium",8591]
["8.24","Medium",8592]
["8.25","Very High",8593]
["8.26","High",8594]
["8.27","Medium",8595]
["8.28","Medium",8596]
["8.29","High",8598]
["8.3","Very High",8571]
["8.30","High",8599]
["8.31","High",8600]
["8.32","Low",8601]
["8.33","Medium",8602]
["8.34","High",8603]
["8.35","Medium",8604]
["8.36","Medium",8605]
["8.37","High",8607]
["8.38","Medium",8608]
["8.39","Medium",8609]
["8.4","Medium",8572]
["8.40","High",8610]
["8.41","Medium",8611]
["8.42","Medium",8612]
["8.43","Very High",8613]
["8.44","High",8615]
["8.45","High",8616]
["8.46","Very High",8617]
["8.47","Very High",8618]
["8.48","Medium",8619]
["8.49","High",8620]
["8.5","Very High",8573]
["8.50","Medium",8621]
["8.51","Low",8622]
["8.52","Low",8623]
["8.53","Low",8624]
["8.54","High",8625]
["8.55","Low",11182]
["8.56","Medium",11183]
["8.57","Medium",11184]
["8.58","High",11185]
["8.59","High",11186]
["8.6","Medium",8574]
["8.60","High",11187]
["8.61","Medium",11188]
["8.62","Very High",11189]
["8.63","High",11190]
["8.64","Medium",11191]
["8.65","Low",11192]
["8.66","High",11193]
["8.67","High",11194]
["8.68","High",11195]
["8.69","Medium",11196]
["8.7","High",8575]
["8.70","Medium",11197]
["8.71","Very High",11198]
["8.72","Medium",11199]
["8.73","Medium",11200]
["8.74","High",11201]
["8.75","Medium",11202]
["8.76","Medium",11203]
["8.77","Medium",11204]
["8.78","Medium",11205]
["8.79","Medium",11206]
["8.8","Medium",8576]
["8.80","Medium",11207]
["8.81","Low",11208]
["8.82","Medium",11209]
["8.83","Low",11210]
["8.84","Low",11211]
["8.85","Medium",11212]
["8.86","Medium",11213]
["8.87","Medium",11214]
["8.88","Low",11215]
["8.89","High",11216]
["8.9","High",8577]
["8.90","High",11217]
["8.91","High",11218]
["8.92","Medium",11219]
["8.93","Low",11220]
["8.94","Low",11221]
["8.95","Medium",11222]
["8.96","Medium",11223]
["8.97","Low",11224]
["8.98","High",11225]
["8.99","Medium",11226]
["9.1","Low",8390]
["9.10","Medium",8399]
["9.11","Medium",8400]
["9.12","Medium",8401]
["9.13","Low",8402]
["9.14","Medium",8403]
["9.15","Medium",8404]
["9.16","High",8405]
["9.17","High",8406]
["9.18","Low",8407]
["9.19","Low",8408]
["9.2","Very High",8391]
["9.20","Medium",8409]
["9.21","Medium",8410]
["9.22","Low",8411]
["9.23","Low",8412]
["9.24","Medium",8413]
["9.25","Low",8414]
["9.26","Low",8415]
["9.27","Low",8416]
["9.28","Medium",8417]
["9.29","Low",8418]
["9.3","Very High",8392]
["9.4","High",8393]
["9.5","High",8394]
["9.6","Low",8395]
["9.7","Medium",8396]
["9.8","Medium",8397]
["9.9","Medium",8398]
["9.99","High",8419]

{"sheet":"Equipment_list","index":7,"n_rows":28,"n_cols":3,"rows_kept":28,"cut":false,"hidden":true,"merged":[]}
["TITLE","Equipment_list_description","ID"]
["Accommodation",null,12]
["Cargo Mach.",null,13]
["Critical Equip.",null,16]
["Deck - Machinery",null,18]
["Deck - Mooring Machinery",null,15]
["Deck - Pipe / Fittings",null,20]
["Documentation",null,21]
["E/R - Air Comp.",null,8]
["E/R - Aux. Engine",null,4]
["E/R - Aux. Mach.",null,7]
["E/R - Boiler",null,5]
["E/R - Main Engine",null,3]
["E/R - Pipes/ valves & fittings",null,9]
["E/R - Pumps",null,32]
["E/R - Purifier",null,6]
["Elect. Mach. & Equip.",null,10]
["Hull & Tanks",null,19]
["Inert Gas",null,14]
["LSA / FFA",null,17]
["Miscellaneous",null,22]
["Navigation - DGPS / EPFS / AIS",null,28]
["Navigation - ECDIS",null,25]
["Navigation - Echo Sounder / Speed Log",null,26]
["Navigation - GMDSS & Communication",null,23]
["Navigation - Others",null,11]
["Navigation - RADAR",null,24]
["Navigation - VDR / BNWAS",null,30]

{"sheet":"PSC_MOU","index":8,"n_rows":11,"n_cols":3,"rows_kept":11,"cut":false,"hidden":true,"merged":[]}
["TITLE","PSC_MOU_description","ID"]
["Asia and the Pacific",null,2]
["Caribbean",null,4]
["Europe and the North Atlantic",null,1]
["Latin America",null,3]
["The Black Sea region",null,6]
["The Indian Ocean",null,8]
["The Mediterranean",null,7]
["The Riyadh MoU",null,9]
["USCG",null,10]
["West and Central Africa",null,5]

{"sheet":"Inspection_type","index":9,"n_rows":13,"n_cols":2,"rows_kept":13,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Bunkering Audit",14]
["Cargo Audit",17]
["Engineering Audit",16]
["ISM Audit",2]
["ISPS Audit",3]
["IT Audit",10]
["MLC Audit",1]
["Mooring Audit",9]
["Nav Audit / Verification",8]
["Onboard Training",18]
["Ship Staff Insp.",15]
["Suptd. Insp.",13]

{"sheet":"Deficiency_Cause","index":10,"n_rows":8,"n_cols":3,"rows_kept":8,"cut":false,"hidden":true,"merged":[]}
["TITLE","Deficiency_Cause_description","ID"]
["Behaviour Based",null,1]
["Equipment Related",null,4]
["External Factors",null,5]
["Human Error",null,7]
["Inappropriate Procedure",null,8]
["Industry Issue",null,6]
["Knowledge Based",null,3]

{"sheet":"Observer_code","index":11,"n_rows":3,"n_cols":3,"rows_kept":3,"cut":false,"hidden":true,"merged":[]}
["TITLE","Observer_code_description","ID"]
["Owner / Marine / Tech. Suptd.",null,3]
["Ship Staff",null,2]

{"sheet":"Status_code","index":12,"n_rows":6,"n_cols":3,"rows_kept":6,"cut":false,"hidden":true,"merged":[]}
["TITLE","Status_code_description","ID"]
["Completed",null,6]
["Deferred to D D",null,5]
["In progress",null,3]
["Not Started",null,2]
["Waiting spare",null,4]

{"sheet":"PSC_ref_no","index":13,"n_rows":19,"n_cols":2,"rows_kept":19,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Alarms",9]
["Cargo operations including equipment",7]
["Certificates & Documentation",2]
["Dangerous Goods",13]
["Emergency Systems",5]
["Fire safety",8]
["ISM",16]
["ISPS",17]
["Life saving appliances",12]
["MLC, 2006",18]
["Other",19]
["Pollution Prevention",15]
["Propulsion and auxiliary machinery",14]
["Radio communication",6]
["Safety of Navigation",11]
["Structural condition",3]
["Water/Weathertight condition",4]
["Working and Living Conditions",10]

{"sheet":"Risk_value_of_obs","index":14,"n_rows":1,"n_cols":2,"rows_kept":1,"cut":false,"hidden":true,"merged":[]}
["Risk Value of observation","ID"]

{"sheet":"Year","index":15,"n_rows":18,"n_cols":1,"rows_kept":18,"cut":false,"hidden":true,"merged":[]}
["Year"]
[2014]
[2015]
[2016]
[2017]
[2018]
[2019]
[2020]
[2021]
[2022]
[2023]
[2024]
[2025]
[2026]
[2027]
[2028]
[2029]
[2030]

{"sheet":"Month","index":16,"n_rows":13,"n_cols":1,"rows_kept":13,"cut":false,"hidden":true,"merged":[]}
["Month"]
["Jan"]
["Feb"]
["Mar"]
["Apr"]
["May"]
["Jun"]
["Jul"]
["Aug"]
["Sep"]
["Oct"]
["Nov"]
["Dec"]

{"sheet":"Date_","index":17,"n_rows":32,"n_cols":1,"rows_kept":32,"cut":false,"hidden":true,"merged":[]}
["Date"]
["01"]
["02"]
["03"]
["04"]
["05"]
["06"]
["07"]
["08"]
["09"]
[10]
[11]
[12]
[13]
[14]
[15]
[16]
[17]
[18]
[19]
[20]
[21]
[22]
[23]
[24]
[25]
[26]
[27]
[28]
[29]
[30]
[31]

{"sheet":"Sheet1","index":18,"n_rows":24,"n_cols":6,"rows_kept":24,"cut":false,"hidden":true,"merged":[]}
[]
[null,"ID","E",null,"Date Recorded",1]
[null,"UNIQUE ID","F",null,"Type of Deficiency",2]
[1,"Date Recorded","G",null,"Observer code",3]
["ignore","Vessel Type","H",null,"Type of Inspection",4]
[null,"Internal / External","I",null,"Description of Deficiency",5]
[null,"Drydock","J",null,"Equipment Categories",6]
[null,"Information Sharing","K",null,"Area of Observation",7]
[null,"Critical_item","L",null,"Deficiency Cause",8]
[null,"Deficiency Type","M",null,"VIQ Ref Number",9]
[null,"Deficiency Cause","N",null,"Risk Value of Obs",10]
[null,"Inspection Type","O",null,"PSC Ref Number",11]
[null,"Equipments","P",null,"PSC MOU ID",12]
[null,"VIQ Reference Number","Q",null,"Action Taken or Required",13]
[null,"Risk Value of the observation","R",null,"Target Date",14]
[null,"PSC Reference Number","S",null,"PO Ref No.",15]
[null,"PSC MOU","T",null,"Status Code",16]
[null,"Observer Code","U",null,"Date Completed",17]
[null,"Target Date","V",null,"Drydock",18]
[null,"Status Code","W",null,"Info Sharing",19]
[null,"Description of Deficiency","X",null,"Critical Item Flag",20]
[null,"Action taken / required","Y",null,"Audit Type",21]
[null,"PO ref no","Z"]
[null,"Date completed","AA"]

{"sheet":"Ship_information","index":19,"n_rows":2,"n_cols":3,"rows_kept":2,"cut":false,"hidden":true,"merged":[]}
["Ship_ID","Ship_Name","FILE_NAME"]
["50","DHT PEONY (24-11-2020)","50_1606871169366.xlsm"]

{"sheet":"External_Deficiency_type","index":20,"n_rows":5,"n_cols":3,"rows_kept":5,"cut":false,"hidden":true,"merged":[]}
["TITLE","Type of deficiency_description","ID"]
["Condn of Class / Memo",null,5]
["Defect",null,1]
["Non Conformity",null,2]
["Observation",null,3]

{"sheet":"External_Inspection_type","index":21,"n_rows":11,"n_cols":2,"rows_kept":11,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Cargo Audit",17]
["Flag State Insp.",5]
["ISM Audit",2]
["ISPS Audit",3]
["MLC Audit",1]
["Nav Audit / Verification",8]
["OM Insp. (Eg. SIRE / CDI etc.)",6]
["Others (Eg. Insurance etc.)",12]
["PSC Inspection",4]
["Terminal Insp.",11]

{"sheet":"External_Observer_code","index":22,"n_rows":7,"n_cols":3,"rows_kept":7,"cut":false,"hidden":true,"merged":[]}
["TITLE","Observer_code_description","ID"]
["Class Surveyor",null,4]
["FSC Inspector",null,5]
["Others (Eg. Insurance etc.)",null,9]
["PSC Insp.",null,6]
["SIRE / CDI Insp.",null,8]
["Terminal Insp.",null,7]

{"sheet":"Sheet Version","index":23,"n_rows":2,"n_cols":2,"rows_kept":2,"cut":false,"hidden":true,"merged":[]}
["Version","Title"]
["2.0","Version 2.0"]