{"text_format":"1","workbook":"xlsx","n_sheets":24,"sheets":["Mainsheet","Completed","Calc","Areaofobs","Vessel_type","Deficiency_type","VIQrefno","Equipment_list","PSC_MOU","Inspection_type","Deficiency_Cause","Observer_code","Status_code","PSC_ref_no","Risk_value_of_obs","Year","Month","Date_","Sheet1","Ship_information","External_Deficiency_type","External_Inspection_type","External_Observer_code","Sheet Version"],"not_rendered":{"charts":0,"images":5,"macros":1,"external_links":0,"defined_names":12,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Mainsheet","index":0,"n_rows":22,"n_cols":28,"rows_kept":22,"cut":false,"hidden":false,"merged":[[10,8,10,9],[10,12,10,13],[12,6,12,27],[8,6,8,27]]}
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,"Defect - Damage Monitoring Sheet"]
[]
[null,null,null,null,null,null,null,"Date of Report","2020-07-15",null,null,"Ship Name","AZIMUTH (01-07-2020)"]
[]
[null,null,null,null,null,null,"VERSION : 2.0"]
[]
[]
[]
[null,null,null,null,"ID","UNIQUE ID","Date Recorded","Type of Deficiency","Observer code","Type of Inspection","Description of Deficiency","Equipment Categories","Area of Observation","Deficiency Cause","VIQ Ref Number","Risk Value of Obs","PSC Ref Number","PSC MOU ID","Action Taken or Required","Target Date","PO Ref No.","Status Code","Date Completed","Drydock","Info Sharing","Critical Item","Audit Type","Superintendent Remarks"]
[null,null,null,null,7927,"98_Thu Dec 12 2019 15:07:43 GMT+0000 (Coordinated Universal Time)","2019-11-18","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","2 nos side longitudinal observed to be buckled on frame no 45 in 4s WBT","Hull & Tanks","Structural Condn. / WT integrity ","Human Error","11.1","High","","","DD Job- Transferred to REFMAN. Job N. S-7.1","2022-07-20","","Deferred to D D",null,"No","No","No","Internal","Vessel to raise drydock specs and include it in REFMAN with all relevant drawings/description. Provide REFMAN no."]
[null,null,null,null,12160,"98_30/4/2020 6:27:58 PM","2020-04-04","Defect,Observation","Ship Staff","Ship Staff Insp.","CARGO RESIDUE OIL TANK","Elect. Mach. & Equip.,Inert Gas","Cargo / Ballast Systems","Equipment Related,External Factors",8.17,"Low","Not Applicable","Not Applicable","REED SWITCH REPLACED BUT STILL IN ERROR","2020-07-20","RO200170 RECEIVED","In progress",null,"No","No","No","Internal","Spares will be connected at Singapore."]
[null,null,null,null,null,"98_12/8/2020 1:28:51 PM","2020-07-19","Defect,Other","Ship Staff","Ship Staff Insp.","BOTH FWD AND AFT ICCP SYSTEM IS GIVING UNDER PROTECTION ALARM","Hull & Tanks","Structural Condn. / WT integrity ","Equipment Related",null,null,"Not Applicable","Not Applicable","AS PER MAKER INSTRUCTIONS RENEWAL OF ANODE AND REFERENCE ELECTRODS ARE REQUIRED.","2020-09-07",null,"In progress",null,"No",null,null,"Internal"]
[null,null,null,null,null,"98_4/10/2020 5:46:21 AM","2020-09-05","Defect","Ship Staff","Ship Staff Insp.","Differential pressure type flow meter not showing proper reading","E/R - Aux. Engine,E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related",null,null,"Not Applicable","Not Applicable","flow indication is not working ","2021-01-31","AZIM200288","Waiting spare",null,"No",null,null,"Internal"]
[null,null,null,null,null,"98_4/10/2020 5:52:22 AM","2020-09-06","Defect","Ship Staff","Ship Staff Insp.","M/E & A/E viscosity controller not working properly","E/R - Aux. Engine,E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related",null,null,"Not Applicable","Not Applicable","Speed reducer is not working for both A/E and M/E","2021-01-31","AZIM200292","Waiting spare",null,"No",null,null,"Internal"]

{"sheet":"Completed","index":1,"n_rows":218,"n_cols":28,"rows_kept":218,"cut":false,"hidden":false,"merged":[[10,8,10,9],[10,12,10,13],[12,6,12,27],[8,6,8,27]]}
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,"Defect - Damage Monitoring Sheet"]
[]
[null,null,null,null,null,null,null,"Date of Report","01-Jul-2020",null,null,"Ship Name","AZIMUTH (01-07-2020)"]
[]
[null,null,null,null,null,null,"VERSION : 2.0"]
[]
[]
[]
[null,null,null,null,"ID","UNIQUE ID","Date Recorded","Type of Deficiency","Observer code","Type of Inspection","Description of Deficiency","Equipment Categories","Area of Observation","Deficiency Cause","VIQ Ref Number","Risk Value of Obs","PSC Ref Number","PSC MOU ID","Action Taken or Required","Target Date","PO Ref No.","Status Code","Date Completed","Drydock","Info Sharing","Critical Item","Audit Type","Superintendent Remarks"]
[null,null,null,null,7898,"98_Thu Dec 12 2019 09:33:49 GMT+0000 (Coordinated Universal Time)","2019-10-18","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Hydrants for COW line to be blanked","Deck - Pipe / Fittings","Cargo / Ballast Systems","Human Error","8.34","High","","","Cow lines hydrant to be blanked","2020-03-15","","Completed","2020-03-11","No","No","No","Internal"]
[null,null,null,null,7950,"98_Sun Dec 08 2019 09:15:33 GMT+0000 (Coordinated Universal Time)","2019-10-27","Breakdown","Ship Staff","Ship Staff Insp.","Galley Hot Plate # 2 out of order","Miscellaneous","Eng. / Strg. Comp.","Human Error,Inappropriate Procedure","","","","","Need to be renewed.","2020-01-10","","Completed","2019-12-09","No","No","No","Internal"]
[null,null,null,null,7848,"98_Sun Dec 08 2019 09:12:04 GMT+0000 (Coordinated Universal Time)","2019-10-27","Defect","Ship Staff","Ship Staff Insp.","Bunker Tank Vent Head Mesh in Damaged Condition.","Miscellaneous","MARPOL Related","Human Error","11.7","High","","","Vent Head Checked and Found Satisfactory","2020-04-30","","Completed","2020-04-19","No","No","No","Internal"]
[null,null,null,null,7949,"98_Sun Dec 08 2019 09:22:23 GMT+0000 (Coordinated Universal Time)","2019-10-28","Defect","Ship Staff","Ship Staff Insp.","Aux boiler Smoke Density Sensor Faulty","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","Need to be Renewed.","2020-01-15","","Completed","2019-12-09","No","No","No","Internal"]
[null,null,null,null,7968,"98_Mon Aug 12 2019 09:24:26 GMT+0000 (Coordinated Universal Time)","2019-10-28","Defect","Ship Staff","Ship Staff Insp.","Incinerator Door Refractory in Damaged Condition.","Miscellaneous","Eng. / Strg. Comp.","Human Error","10.32","Very High","","","Door Refractory renewed.","2019-12-20","","Completed","2019-12-13","No","No","No","Internal"]
[null,null,null,null,7849,"98_Sun Dec 08 2019 09:20:23 GMT+0000 (Coordinated Universal Time)","2019-10-28","Defect","Ship Staff","Ship Staff Insp.","#4 S Cargo Tank IG Pressure Sensor Faulty ","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.23","Medium","","","Service Engineer attended the vessel and calibration/servicing carried out.found satisfactory","2020-04-30","205015","Completed","2020-04-02","No","No","No","Internal"]
[null,null,null,null,7850,"98_Sun Dec 08 2019 09:26:30 GMT+0000 (Coordinated Universal Time)","2019-10-28","Defect","Ship Staff","Ship Staff Insp.","Main Engine VIT Out Of Order","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related,Human Error","10.32","Very High","","","PCB Installed,all the setting carried out as per makers instructions,found satisfactory","2020-04-30","","Completed","2020-03-27","No","No","No","Internal"]
[null,null,null,null,7969,"98_Sun Dec 08 2019 09:29:14 GMT+0000 (Coordinated Universal Time)","2019-10-29","Defect","Ship Staff","Ship Staff Insp.","Sludge and Bilge Tank Self Closing Sounding device malfunctioning.","Miscellaneous","MARPOL Related","Equipment Related,Human Error","10.26","High","","","Repaired Carried out","2019-12-20","","Completed","2019-12-13","No","No","No","Internal"]
[null,null,null,null,7970,"98_Mon Aug 12 2019 09:38:48 GMT+0000 (Coordinated Universal Time)","2019-10-29","Defect","Ship Staff","Ship Staff Insp.","IG Overboard Line NRV Check Valve body cleaking for sea water.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related,Human Error","10.32","Very High","","","Valve renewed.","2019-12-20","","Completed","2019-12-11","No","No","No","Internal"]
[null,null,null,null,7971,"98_Mon Aug 12 2019 09:49:27 GMT+0000 (Coordinated Universal Time)","2019-10-29","Defect","Ship Staff","Ship Staff Insp.","STBD Bridge Wing Rudder angle and ME RPM indicator showing Erratic Reading","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","Checked and found satisfactory","2020-01-30","","Completed","2019-12-09","No","No","No","Internal"]
[null,null,null,null,8744,"98_Sun Dec 08 2019 09:38:47 GMT+0000 (Coordinated Universal Time)","2019-10-29","Defect","Ship Staff","Ship Staff Insp.","IG Overboard Line NRV Check Valve body cleaking for sea water.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related,Human Error","10.32","Very High","","","Valve renewed.","2019-12-20","","Completed","2019-12-11","No","No","No","Internal"]
[null,null,null,null,7851,"98_Mon Aug 12 2019 09:31:06 GMT+0000 (Coordinated Universal Time)","2019-10-29","Defect","Ship Staff","Ship Staff Insp.","Fresh Water Sterilizer in non operational.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related,Human Error","10.32","Very High","","","Repaired and operational","2020-03-31","","Completed","2020-03-01","No","No","No","Internal"]
[null,null,null,null,7852,"98_Sun Dec 08 2019 09:33:48 GMT+0000 (Coordinated Universal Time)","2019-10-29","Defect","Ship Staff","Ship Staff Insp.","Main Engine Fuel Oil backwash Filter Leaking for oil from body.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related,Human Error","10.32","Very High","","","All the O-ring  Renewed.","2019-12-20","","Completed","2019-12-11","No","No","No","Internal"]
[null,null,null,null,7854,"98_Sun Dec 08 2019 09:46:05 GMT+0000 (Coordinated Universal Time)","2019-10-29","Defect","Ship Staff","Ship Staff Insp.","Engine Room Bilge Well Gratings are missing","E/R - Pipes/ valves & fittings","Structural Condn. / WT integrity ","Human Error","10.29","Medium","","","Fabricate and installed.","2019-12-30","","Completed","2019-12-28","No","No","No","Internal"]
[null,null,null,null,7855,"98_Sun Dec 08 2019 16:26:11 GMT+0000 (Coordinated Universal Time)","2019-10-29","Defect","Ship Staff","Ship Staff Insp.","Aux Boiler FO Burn Pump#1 Seal Leaking","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related,Human Error","10.32","Very High","","","Pump Overhauled,Tried out and found Satisfactory.","2020-03-31","","Completed","2020-02-08","No","No","No","Internal"]
[null,null,null,null,7856,"98_Sun Dec 08 2019 16:27:59 GMT+0000 (Coordinated Universal Time)","2019-10-29","Defect","Ship Staff","Ship Staff Insp.","Deck Air Compressor underrated condition.","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related,Human Error","10.32","Very High","","","Overhauled.","2020-01-20","PO195032","Completed","2020-01-16","No","No","No","Internal"]
[null,null,null,null,7857,"98_Sun Dec 08 2019 16:34:10 GMT+0000 (Coordinated Universal Time)","2019-10-29","Critical Equipment,Defect","Ship Staff","Ship Staff Insp.","EM.Gen.QCV Remote Handle in Corroded Condition.","Critical Equip.","Emgcy. Systems","Equipment Related,Human Error,Inappropriate Procedure","10.32","Very High","","","chipped and painted","2020-02-25","","Completed","2020-02-22","No","No","No","Internal"]
[null,null,null,null,7858,"98_Sun Dec 08 2019 16:37:43 GMT+0000 (Coordinated Universal Time)","2019-10-29","Defect","Ship Staff","Ship Staff Insp.","Aux Blr FO Burn Pump #1 Seal pot Leaking","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related,Human Error,Inappropriate Procedure","10.32","Very High","","","Seal Pot rubber ring renewed.","2020-03-31","PO190102","Completed","2020-02-08","No","No","No","Internal"]
[null,null,null,null,7859,"98_Sun Dec 08 2019 16:39:50 GMT+0000 (Coordinated Universal Time)","2019-10-29","Defect","Ship Staff","Ship Staff Insp.","HFO Bunker Tank Manifold PR and Temp gauges not in place.","Deck - Pipe / Fittings","MARPOL Related","Equipment Related,Human Error,Inappropriate Procedure","6.8","High","","","Fabrication to be carried out on Bunker Pipe.","2020-05-31","","Completed","2020-05-15","No","No","No","Internal"]
[null,null,null,null,7860,"98_Mon Aug 12 2019 16:43:55 GMT+0000 (Coordinated Universal Time)","2019-10-29","Defect","Ship Staff","Ship Staff Insp.","Provision Crane 2.5 T Hook Latch in broken, wire in damaged condition and winch hoist motor break pad in damaged..","Deck - Machinery","Eng. / Strg. Comp.","Equipment Related,Human Error,Inappropriate Procedure","8.73","Medium","","","Hoisting motor brake renewed,wire renewed,found satisfactory","2020-04-30","PO190099","Completed","2020-04-02","No","No","No","Internal"]
[null,null,null,null,null,"98_Sun Dec 08 2019 09:44:07 GMT+0000 (Coordinated Universal Time)","2019-10-29","Defect","Ship Staff","Ship Staff Insp.","MAIN ENGINE PERFORMANCE KIT NOT OPERATIONAL.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","KIT RECEIVED.","2020-07-31","RO200041","Completed","2020-07-11","No",null,null,"Internal"]
[null,null,null,null,7977,"98_Mon Aug 12 2019 17:04:07 GMT+0000 (Coordinated Universal Time)","2019-10-30","Defect","Ship Staff","Ship Staff Insp.","ME FO Booster Pump Pr Gauges are Faulty","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related,Human Error,Inappropriate Procedure","10.32","Very High","","","Need to be renewed.","2019-12-29","","Completed","2019-12-13","No","No","No","Internal"]
[null,null,null,null,8745,"98_Sun Dec 08 2019 17:04:06 GMT+0000 (Coordinated Universal Time)","2019-10-30","Defect","Ship Staff","Ship Staff Insp.","ME FO Booster Pump Pr Gauges are Faulty","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related,Human Error,Inappropriate Procedure","10.32","Very High","","","Renewed.","2019-12-29","","Completed","2019-12-13","No","No","No","Internal"]
[null,null,null,null,7978,"98_Mon Aug 12 2019 17:06:25 GMT+0000 (Coordinated Universal Time)","2019-10-30","Defect","Ship Staff","Ship Staff Insp.","Aux Blr Pilot Burner Pump Pr Gauges Faulty","E/R - Boiler","","Equipment Related,Human Error,Inappropriate Procedure","10.32","Very High","","","Need to be renewed.","2019-12-30","","Completed","2019-12-14","No","No","No","Internal"]
[null,null,null,null,8746,"98_Sun Dec 08 2019 17:06:25 GMT+0000 (Coordinated Universal Time)","2019-10-30","Defect","Ship Staff","Ship Staff Insp.","Aux Blr Pilot Burner Pump Pr Gauges Faulty","E/R - Boiler","","Equipment Related,Human Error,Inappropriate Procedure","10.32","Very High","","","Renewed.","2019-12-30","","Completed","2019-12-14","No","No","No","Internal"]
[null,null,null,null,8747,"98_Mon Aug 12 2019 16:55:41 GMT+0000 (Coordinated Universal Time)","2019-10-30","Critical Equipment,Defect","Ship Staff","Ship Staff Insp.","Both Foam Tank gauge glass slightley leaking for foam","LSA / FFA","Emgcy. Systems","Behaviour Based,Human Error,Inappropriate Procedure","10.18","High","","","Both the gauge glass leakages rectified.","2019-12-25","","Completed","2019-12-20","No","No","No","Internal"]
[null,null,null,null,7861,"98_Sun Dec 08 2019 16:45:45 GMT+0000 (Coordinated Universal Time)","2019-10-30","Defect","Ship Staff","Ship Staff Insp.","Provision crane 0.9T Wire/hook and Sheves in poor condition ","Deck - Machinery","Eng. / Strg. Comp.","Equipment Related,Human Error,Inappropriate Procedure","8.73","Medium","","","blocked repaired","2020-02-29","","Completed","2020-02-25","No","No","No","Internal"]
[null,null,null,null,7862,"98_Sun Dec 08 2019 16:50:14 GMT+0000 (Coordinated Universal Time)","2019-10-30","Defect","Ship Staff","Ship Staff Insp.","ER Blower Intake Gratings are in damage and corroded condition","Deck - Machinery","General Appearance","Equipment Related,Human Error,Inappropriate Procedure","10.32","Very High","","","chipped and fabricate for damaged one.","2020-01-15","","Completed","2020-01-04","No","No","No","Internal"]
[null,null,null,null,7863,"98_Sun Dec 08 2019 16:55:41 GMT+0000 (Coordinated Universal Time)","2019-10-30","Critical Equipment,Defect","Ship Staff","Ship Staff Insp.","Both Foam Tank gauge glass slightley leaking for foam","LSA / FFA","Emgcy. Systems","Behaviour Based,Human Error,Inappropriate Procedure","10.18","High","","","repaired.","2019-12-25","","Completed","2019-12-24","No","No","No","Internal"]
[null,null,null,null,7864,"98_Sun Dec 08 2019 16:58:01 GMT+0000 (Coordinated Universal Time)","2019-10-30","Defect","Ship Staff","Ship Staff Insp.","Both ME Air Cooler and EGB U type Manometer not in place.","E/R - Boiler,E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related,Human Error,Inappropriate Procedure","10.32","Very High","",""," installed new one.","2020-01-30","","Completed","2020-01-17","No","No","No","Internal"]
[null,null,null,null,7979,"98_Mon Aug 12 2019 17:11:18 GMT+0000 (Coordinated Universal Time)","2019-10-31","Defect","Ship Staff","Ship Staff Insp.","Lub Oil Transfer Pump Pr Gauges Faulty","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related,Human Error,Inappropriate Procedure","10.32","Very High","","","Renewed.","2019-12-30","","Completed","2019-12-14","No","No","No","Internal"]
[null,null,null,null,7865,"98_Sun Dec 08 2019 17:09:56 GMT+0000 (Coordinated Universal Time)","2019-10-31","Defect","Ship Staff","Ship Staff Insp.","Aux Blr Local FO Pr gauge connection Leaking for Oil.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related,Human Error,Inappropriate Procedure","10.32","Very High","","","tightened.","2019-12-31","","Completed","2019-12-29","No","No","No","Internal"]
[null,null,null,null,7866,"98_Sun Dec 08 2019 17:14:38 GMT+0000 (Coordinated Universal Time)","2019-10-31","Defect","Ship Staff","Ship Staff Insp.","Auxiliary Engine # 3 Local temp and TC Oil Pr gauges Faulty","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related,Human Error,Inappropriate Procedure","10.32","Very High","","","Renewed.","2019-12-31","PO190032","Completed","2019-12-29","No","No","No","Internal"]
[null,null,null,null,7867,"98_Sun Dec 08 2019 17:18:09 GMT+0000 (Coordinated Universal Time)","2019-10-31","Defect","Ship Staff","Ship Staff Insp.","Auxiliary Engine #1 FO pr Gauge Faulty","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related,Human Error,Inappropriate Procedure","10.32","Very High","","","Renewed.","2019-12-31","PO190032","Completed","2019-12-29","No","No","No","Internal"]
[null,null,null,null,7869,"98_Sun Dec 08 2019 17:21:19 GMT+0000 (Coordinated Universal Time)","2019-10-31","Defect","Ship Staff","Ship Staff Insp.","F.W Hydrophore Air Line Filter in damaged condition","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related,Human Error,Inappropriate Procedure","10.32","Very High","","","Renewed.","2019-12-31","","Completed","2019-12-29","No","No","No","Internal"]
[null,null,null,null,7871,"98_Sun Dec 08 2019 17:26:21 GMT+0000 (Coordinated Universal Time)","2019-10-31","Defect","Ship Staff","Ship Staff Insp.","Funnel Flaps some of the Sealing face found in damaged condition","Critical Equip.","Emgcy. Systems","Equipment Related,Human Error,Inappropriate Procedure","10.32","Very High","","","repaired.","2019-12-30","","Completed","2019-12-25","No","No","No","Internal"]
[null,null,null,null,7980,"98_Mon Aug 12 2019 17:34:03 GMT+0000 (Coordinated Universal Time)","2019-11-02","Defect","Ship Staff","Ship Staff Insp.","Sludge Pump Pressure Gauges Connection in opaque condition.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related,Human Error,Inappropriate Procedure","10.32","Very High","","","Renewed.","2019-12-31","","Completed","2019-12-13","No","No","No","Internal"]
[null,null,null,null,8748,"98_Mon Aug 12 2019 17:19:49 GMT+0000 (Coordinated Universal Time)","2019-11-02","Defect","Ship Staff","Ship Staff Insp.","Auxiliary Engine# 2 Tachometer Gauge Faulty","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related,Human Error,Inappropriate Procedure","10.32","Very High","","","Renewed.","2019-12-31","PO190032","Completed","2019-12-22","No","No","No","Internal"]
[null,null,null,null,7981,"98_Mon Dec 09 2019 15:03:01 GMT+0000 (Coordinated Universal Time)","2019-11-02","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Blr Wtr Circulating Pump # 1 Pressure Gauges Malfunctioning","Miscellaneous","Eng. / Strg. Comp.","Equipment Related,Human Error,Inappropriate Procedure","10.32","Very High","","","renewed","2019-12-31","","Completed","2019-12-14","No","No","No","Internal"]
[null,null,null,null,8756,"98_Thu Sep 12 2019 15:05:24 GMT+0000 (Coordinated Universal Time)","2019-11-02","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Not arrange chemical Locker for Alkali and Acid Chemicals","Miscellaneous","Eng. / Strg. Comp.","Equipment Related,Human Error,Inappropriate Procedure","10.29","Medium","","","Arranged and Secured","2020-01-10","","Completed","2019-12-17","No","No","No","Internal"]
[null,null,null,null,7872,"98_Mon Aug 12 2019 17:28:20 GMT+0000 (Coordinated Universal Time)","2019-11-02","Defect","Ship Staff","Ship Staff Insp.","AC Plant Evaporator is underrated condition.","Accommodation","Eng. / Strg. Comp.","Equipment Related,Human Error,Inappropriate Procedure","10.32","Very High","","","Evaporator Renewed","2020-04-30","PO195170","Completed","2020-04-04","No","No","No","Internal"]
[null,null,null,null,7873,"98_Sun Dec 08 2019 17:31:01 GMT+0000 (Coordinated Universal Time)","2019-11-02","Defect","Ship Staff","Ship Staff Insp.","Main Engine Unit # 2 Camshaft Bush Leaking for Oil.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related,Inappropriate Procedure","10.32","Very High","","","Vessel received the spare parts and leakages are rectified.","2020-03-31","","Completed","2020-03-30","No","No","No","Internal"]
[null,null,null,null,7874,"98_Sun Dec 08 2019 17:41:36 GMT+0000 (Coordinated Universal Time)","2019-11-02","Defect","Ship Staff","Ship Staff Insp.","RO filter out of operation.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related,Human Error,Inappropriate Procedure","10.32","Very High","","","Checked and found discarded condition","2020-01-31","","Completed","2020-01-02","No","No","No","Internal"]
[null,null,null,null,7880,"98_Mon Dec 09 2019 15:05:24 GMT+0000 (Coordinated Universal Time)","2019-11-02","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Not arrange chemical Locker for Alkali and Acid Chemicals","Miscellaneous","Eng. / Strg. Comp.","Equipment Related,Human Error,Inappropriate Procedure","10.29","Medium","","","Arranged the Locker.","2020-01-10","","Completed","2019-12-18","No","No","No","Internal"]
[null,null,null,null,null,"98_Sun Dec 08 2019 17:19:49 GMT+0000 (Coordinated Universal Time)","2019-11-02","Defect","Ship Staff","Ship Staff Insp.","AUXILIARY ENGINE #2 TACHOMETER GAUGE FAULTY","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related,Human Error,Inappropriate Procedure",10.32,"Very High","Not Applicable","Not Applicable","RO Not Received and Tachometer Wire were in damaged condition.","2020-07-30","RO200067","Completed","2020-07-16","No",null,null,"Internal"]
[null,null,null,null,7876,"98_Sun Dec 08 2019 17:46:25 GMT+0000 (Coordinated Universal Time)","2019-11-03","Defect","Ship Staff","Ship Staff Insp.","Oxy and Acetyle Bottles Hoses clamp in damaged condition.","E/R - Aux. Mach.","General Appearance","Equipment Related,Human Error,Inappropriate Procedure","5.25","Medium","","","Clamp renewed.","2020-02-29","","Completed","2020-01-29","No","No","No","Internal"]
[null,null,null,null,7877,"98_Sun Dec 08 2019 17:48:07 GMT+0000 (Coordinated Universal Time)","2019-11-03","Defect","Ship Staff","Ship Staff Insp.","Lub Oil Cooler S.W. Outlet Flange Connection Leaking.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related,Human Error,Inappropriate Procedure","10.32","Very High","","","Renewed.","2020-01-31","","Completed","2020-01-16","No","No","No","Internal"]
[null,null,null,null,7878,"98_Sun Dec 08 2019 17:51:11 GMT+0000 (Coordinated Universal Time)","2019-11-03","Defect","Ship Staff","Ship Staff Insp.","F.W.Pipe Lines found corroded and leaking.(Steering Gear Room/Accomodation)","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related,Human Error,Inappropriate Procedure","10.32","Very High","","","Renewed.","2019-12-31","","Completed","2019-12-22","No","No","No","Internal"]
[null,null,null,null,null,"98_Mon Aug 12 2019 17:44:41 GMT+0000 (Coordinated Universal Time)","2019-11-03","Defect","Ship Staff","Ship Staff Insp.","GALLEY AC UNIT OUT OF ORDER.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related,Inappropriate Procedure",10.32,"Very High","Not Applicable","Not Applicable","Evaporator Renewed but FAN unit are in damaged condition.","2020-07-30","RO200169","Completed","2020-07-15","No",null,null,"Internal"]
[null,null,null,null,7972,"98_Thu Sep 12 2019 15:14:01 GMT+0000 (Coordinated Universal Time)","2019-11-04","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","#1 ME FO Booster Pump Pressure Gauges in Opaque Condition.","Miscellaneous","General Appearance","Human Error,Inappropriate Procedure","","","","","Need to be renewed.","2020-01-10","","Completed","2019-12-13","No","No","No","Internal"]
[null,null,null,null,7982,"98_Mon Dec 09 2019 15:08:20 GMT+0000 (Coordinated Universal Time)","2019-11-04","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Economiser # 1 and # 2 Pressure Gauges found in broken condition","Miscellaneous","General Appearance","Human Error,Inappropriate Procedure","10.32","Very High","",""," renewed.","2020-01-10","","Completed","2019-12-14","No","No","No","Internal"]
[null,null,null,null,7983,"98_Mon Dec 09 2019 15:17:07 GMT+0000 (Coordinated Universal Time)","2019-11-04","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Sludge Pump Pressure Gauges in Opaque Condition","Miscellaneous","General Appearance","Human Error,Inappropriate Procedure","10.32","Very High","","","renewed.","2020-01-10","","Completed","2019-12-13","No","No","No","Internal"]
[null,null,null,null,7984,"98_Mon Dec 09 2019 15:18:50 GMT+0000 (Coordinated Universal Time)","2019-11-04","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Light around accomodation found in fused condition","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Human Error,Inappropriate Procedure","10.15","Low","",""," renewed.","2020-01-15","","Completed","2019-12-12","No","No","No","Internal"]
[null,null,null,null,7986,"98_Thu Sep 12 2019 19:59:09 GMT+0000 (Coordinated Universal Time)","2019-11-04","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Jacket Water Pump Coupling Guard Missing.","Miscellaneous","General Appearance","Equipment Related,Human Error,Inappropriate Procedure","10.27","Medium","",""," assembled.","2020-01-10","","Completed","2019-12-14","No","No","No","Internal"]
[null,null,null,null,7881,"98_Mon Dec 09 2019 15:06:52 GMT+0000 (Coordinated Universal Time)","2019-11-04","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Grinder Protective Transparent Sheet in Opaque Condition","Miscellaneous","General Appearance","Human Error,Inappropriate Procedure","10.27","Medium","",""," renewed.","2020-01-10","","Completed","2019-12-26","No","No","No","Internal"]
[null,null,null,null,7882,"98_Mon Dec 09 2019 15:10:07 GMT+0000 (Coordinated Universal Time)","2019-11-04","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Protection Guard Missing on Fire Pumps/Main Sea Water Pumps/Scrubber Pumps","Miscellaneous","General Appearance","Human Error,Inappropriate Procedure","10.27","Medium","",""," installed.","2020-01-10","","Completed","2019-12-17","No","No","No","Internal"]
[null,null,null,null,7883,"98_Thu Sep 12 2019 15:15:26 GMT+0000 (Coordinated Universal Time)","2019-11-04","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Motor Protection cover missing from few motors","Miscellaneous","General Appearance","Human Error,Inappropriate Procedure","10.27","Medium","",""," installed.","2020-01-10","","Completed","2020-01-03","No","No","No","Internal"]
[null,null,null,null,7886,"98_Mon Dec 09 2019 20:01:14 GMT+0000 (Coordinated Universal Time)","2019-11-04","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Few Rubber Pad Missing from aluminium ladder.","Miscellaneous","General Appearance","External Factors,Human Error,Inappropriate Procedure","5.47","Medium","",""," installed.","2020-04-30","","Completed","2020-03-31","No","No","No","Internal"]
[null,null,null,null,7870,"98_Sun Dec 08 2019 17:24:22 GMT+0000 (Coordinated Universal Time)","2019-11-05","Critical Equipment,Defect","Ship Staff","Ship Staff Insp.","Sewage Plant air Blower out of operation.","Critical Equip.","Eng. / Strg. Comp.","Equipment Related,Human Error,Inappropriate Procedure","10.32","Very High","",""," renewed.","2019-12-31","PO195026","Completed","2019-12-27","No","No","No","Internal"]
[null,null,null,null,8749,"98_23/12/2019 2:35:20 PM","2019-11-16","Non Conformity","Class Surveyor","MLC Audit","Spare Officer A,B and C- Tiles in toilet are broken.","Accommodation","MLC Related","Human Error","11.13","Low","","","New tiles fitted.","2019-12-07","","Completed","2019-12-07","No","No","No","Internal"]
[null,null,null,null,8750,"98_23/12/2019 2:41:00 PM","2019-11-16","Defect","Class Surveyor","MLC Audit","Upper deck common toilet, laundry and changing locker - cleanliness to be maintained","Accommodation","MLC Related","Human Error","11.13","Low","","","Areas cleaned.","2019-12-07","","Completed","2019-12-07","No","No","No","Internal"]
[null,null,null,null,7937,"98_Thu Dec 12 2019 19:02:13 GMT+0000 (Coordinated Universal Time)","2019-11-18","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Fire plan symbol to be corrected","LSA / FFA","Safety / LSA / FFA","Human Error","5.27","Medium","","","To be corrected","2020-02-20","","Completed","2020-02-14","No","No","No","Internal"]
[null,null,null,null,7938,"98_Thu Dec 12 2019 19:04:09 GMT+0000 (Coordinated Universal Time)","2019-11-18","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Forward Life raft light missing","LSA / FFA","Safety / LSA / FFA","Human Error","5.27","Medium","","","New to be ordered","2019-12-10","","Completed","2019-12-25","No","No","No","Internal"]
[null,null,null,null,7941,"98_Thu Dec 12 2019 22:28:39 GMT+0000 (Coordinated Universal Time)","2019-11-18","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","SOPEP inventory to be updated","Miscellaneous","MARPOL Related","Human Error","6.1","Medium","","","Inventory to be taken and updated","2019-12-25","","Completed","2020-01-19","No","No","No","Internal"]
[null,null,null,null,7942,"98_13/12/2019 10:24:23 AM","2019-11-18","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","All fire hose boxes to be inspected","LSA / FFA","Safety / LSA / FFA","Human Error","5.35","Medium","","","Fire boxes to be cleaned & inspected","2019-12-16","","Completed","2020-01-04","No","No","No","Internal"]
[null,null,null,null,7943,"98_13/12/2019 10:27:39 AM","2019-11-18","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Securing strap (1 nos) for EEBD in pump room bottom partially broken","LSA / FFA","Safety / LSA / FFA","Human Error","5.27","Medium","","","Strap to be renewed","2019-12-18","","Completed","2019-12-24","No","No","No","Internal"]
[null,null,null,null,7944,"98_13/12/2019 12:50:31 PM","2019-11-18","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Danger High voltage IMO symbol missing on No-6 group starter box","LSA / FFA","Safety / LSA / FFA","Human Error","","","","","IMO symbol pasted","2020-01-20","","Completed","2020-01-02","No","No","No","Internal"]
[null,null,null,null,7945,"98_13/12/2019 12:53:30 PM","2019-11-18","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Recommend to fabricate storage boxes for EEBD to protect it from environment","LSA / FFA","Safety / LSA / FFA","Human Error","5.27","Medium","","","Vessel fabricated boxes","2020-06-30","","Completed","2020-06-20","No","No","No","Internal","This defect noticed in Nov'19, confirm if same rectified. Update DDL accordingly."]
[null,null,null,null,7946,"98_13/12/2019 12:55:13 PM","2019-11-18","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Discharge hose for foam wheeled extinguisher no-46 nr emergency exit bottom platform have superficial damage","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.27","Medium","","","RENEWED","2020-05-20","AZIM200078","Completed","2020-03-12","No","No","No","Internal"]
[null,null,null,null,7947,"98_13/12/2019 1:47:14 PM","2019-11-18","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Update maintenance plan","Miscellaneous","General Appearance","Human Error","","","","","Maintenance plan file to be prepared and maintained","2020-01-30","","Completed","2020-01-01","No","No","No","Internal"]
[null,null,null,null,7948,"98_13/12/2019 1:52:46 PM","2019-11-18","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Training for PAL to be given to crew","Miscellaneous","MLC Related","Knowledge Based","","","","","Training to be given to all crew members.","2019-12-30","","Completed","2019-12-21","No","No","No","Internal"]
[null,null,null,null,7951,"98_Thu Dec 12 2019 17:29:27 GMT+0000 (Coordinated Universal Time)","2019-11-18","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ODME not recognising USB drive for downloading data","Critical Equip.","MARPOL Related","Equipment Related","","","","","To be reactified","2019-12-15","","Completed","2019-11-21","No","No","No","Internal"]
[null,null,null,null,7952,"98_Thu Dec 12 2019 18:05:58 GMT+0000 (Coordinated Universal Time)","2019-11-18","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Bridge door from accomodation stairway upper hinge broken","Accommodation","General Appearance","Human Error","","","","","To be repaired","2019-12-15","","Completed","2019-12-03","No","No","No","Internal"]
[null,null,null,null,7953,"98_Thu Dec 12 2019 18:08:06 GMT+0000 (Coordinated Universal Time)","2019-11-18","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Air con outlet diffuser cover missing in cabin “2nd Engineer”","Accommodation","General Appearance","Human Error","","","","","To be fixed","2019-12-15","","Completed","2019-12-24","No","No","No","Internal"]
[null,null,null,null,7954,"98_Thu Dec 12 2019 18:10:00 GMT+0000 (Coordinated Universal Time)","2019-11-18","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Hot water Tap is leaking and currently isolated in total 6 cabins (C/E, Oiler-A, Cadet-B, Spare off-C, Spare off-D, Worker cabin)","Accommodation","MLC Related","Human Error","","","","","To be repaired","2019-12-15","","Completed","2019-12-03","No","No","No","Internal"]
[null,null,null,null,7955,"98_Thu Dec 12 2019 18:11:36 GMT+0000 (Coordinated Universal Time)","2019-11-18","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Shower mixer for hot water not working  / Leaking & isolated in total 2 cabins (AB-A, Worker cabin)","Accommodation","MLC Related","Human Error","","","","","To be repaired","2019-12-15","","Completed","2019-12-04","No","No","No","Internal"]
[null,null,null,null,7956,"98_Thu Dec 12 2019 18:14:00 GMT+0000 (Coordinated Universal Time)","2019-11-18","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Bed lamp fixture 1 nos missing from worker cabin (Total there are 4 beds in this cabin)","Accommodation","MLC Related","Human Error","","","","","New bed lamp to be fixed","2019-12-15","","Completed","2019-12-12","No","No","No","Internal"]
[null,null,null,null,7957,"98_Thu Dec 12 2019 18:28:22 GMT+0000 (Coordinated Universal Time)","2019-11-18","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Flooring cement is damaged and will have to be redone in worker cabin","Accommodation","MLC Related","Human Error","","","","","To be repaired","2019-12-15","","Completed","2019-12-04","No","No","No","Internal"]
[null,null,null,null,7958,"98_Thu Dec 12 2019 18:36:09 GMT+0000 (Coordinated Universal Time)","2019-11-18","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Minor damage on bridge wing door coming from stair case","Accommodation","General Appearance","Human Error","","","","","To be repaired","2019-12-15","","Completed","2019-12-03","No","No","No","Internal"]
[null,null,null,null,7959,"98_Thu Dec 12 2019 18:37:57 GMT+0000 (Coordinated Universal Time)","2019-11-18","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Tell tale signs of leakage of water from port hole windows observed cabins","Accommodation","MLC Related","Human Error","","","","","To be repaired","2019-12-15","","Completed","2019-12-04","No","No","No","Internal"]
[null,null,null,null,7960,"98_Thu Dec 12 2019 18:39:25 GMT+0000 (Coordinated Universal Time)","2019-11-18","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Bathroom light fitting cover damaged in 2 cabins","Accommodation","MLC Related","Human Error","","","","","To be changed","2019-12-15","","Completed","2019-12-12","No","No","No","Internal"]
[null,null,null,null,7961,"98_Thu Dec 12 2019 18:41:11 GMT+0000 (Coordinated Universal Time)","2019-11-18","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","2 nos bed lamp in cabin found not working","Accommodation","MLC Related","Human Error","","","","","Lights to be changed","2019-12-15","","Completed","2019-12-03","No","No","No","Internal"]
[null,null,null,null,7962,"98_Thu Dec 12 2019 18:46:13 GMT+0000 (Coordinated Universal Time)","2019-11-18","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Ships name to be marked on life raft and in the identification card","LSA / FFA","Safety / LSA / FFA","Human Error","","","","","Name to be stenciled","2019-11-22","","Completed","2019-11-19","No","No","No","Internal"]
[null,null,null,null,7963,"98_Thu Dec 12 2019 18:48:30 GMT+0000 (Coordinated Universal Time)","2019-11-18","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Eye wash inside chemical, paint locker, Battery room, Boiler chemical area & forecastle store expired","Miscellaneous","General Appearance","Human Error","","","","","Replaced with new one","2019-12-15","","Completed","2019-12-09","No","No","No","Internal"]
[null,null,null,null,7964,"98_Thu Dec 12 2019 18:57:55 GMT+0000 (Coordinated Universal Time)","2019-11-18","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Total 3 nos oars in lifeboat damaged","LSA / FFA","Safety / LSA / FFA","Human Error","","","","","New to be ordered","2019-12-15","","Completed","2019-12-01","No","No","No","Internal"]
[null,null,null,null,7965,"98_Thu Dec 12 2019 22:31:35 GMT+0000 (Coordinated Universal Time)","2019-11-18","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","No-5 foam monitor leaking","LSA / FFA","Safety / LSA / FFA","Human Error","","","","","Valve to be changed","2019-12-15","","Completed","2019-12-09","No","No","No","Internal"]
[null,null,null,null,7966,"98_13/12/2019 1:12:48 PM","2019-11-18","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Shipboard working arrangement to be prepared","Miscellaneous","General Appearance","Human Error","","","","","Working arrangement to be prepared and pasted","2019-11-23","","Completed","2019-11-20","No","No","No","Internal"]
[null,null,null,null,7967,"98_13/12/2019 1:15:50 PM","2019-11-18","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Onboard complaint file to be prepared","Miscellaneous","General Appearance","Human Error","","","","","File to be prepared","2019-12-25","","Completed","2019-11-28","No","No","No","Internal"]
[null,null,null,null,7973,"98_Mon Dec 09 2019 19:46:57 GMT+0000 (Coordinated Universal Time)","2019-11-18","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Intrinisically Safe Phone not operational in Pump Room","Elect. Mach. & Equip.","General Appearance","Human Error,Inappropriate Procedure","5.6","Low","","","Checked and found satisfactory.","2020-01-15","","Completed","2019-12-14","No","No","No","Internal"]
[null,null,null,null,7974,"98_Thu Dec 12 2019 14:26:51 GMT+0000 (Coordinated Universal Time)","2019-11-18","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Anchor wash and educator overboard pipe having soft patches near Hawse pipe penetration on both sides","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","Human Error","11.4","Very High","","","Crack pipes to be renewed","2019-12-15","","Completed","2019-12-13","No","No","No","Internal"]
[null,null,null,null,7975,"98_13/12/2019 1:42:41 PM","2019-11-18","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Prepare mooring matrix","Miscellaneous","Mooring","Human Error","9.2","Very High","","","Mooring matrix to be prepared","2019-12-30","","Completed","2019-12-14","No","No","No","Internal"]
[null,null,null,null,7976,"98_13/12/2019 1:50:48 PM","2019-11-18","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Update gas instrument records","Miscellaneous","Cargo / Ballast Systems","Equipment Related","","","","","Records to be prepared and updated","2020-01-30","","Completed","2019-12-14","No","No","No","Internal"]
[null,null,null,null,7985,"98_Mon Dec 09 2019 19:49:42 GMT+0000 (Coordinated Universal Time)","2019-11-18","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Engine room Workshop Lathe Machine Emergency Swith is non operational.","Elect. Mach. & Equip.","General Appearance","Equipment Related,Human Error,Inappropriate Procedure","10.32","Very High","","","checked and repaired.","2020-01-10","","Completed","2019-12-13","No","No","No","Internal"]
[null,null,null,null,7987,"98_Mon Dec 09 2019 20:03:02 GMT+0000 (Coordinated Universal Time)","2019-11-18","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Bed and Bathroom Lights Missing for Few Cabins","Miscellaneous","General Appearance","Equipment Related,External Factors,Human Error,Inappropriate Procedure","11.13","Low","",""," Repaired & renewed.","2020-01-10","","Completed","2019-12-12","No","No","No","Internal"]
[null,null,null,null,7847,"98_13/12/2019 1:45:12 PM","2019-11-18","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Updated tank inspection records","Hull & Tanks","Cargo / Ballast Systems","Human Error","2.9","Medium","","","COT / BALLAST TANK  inspection records to be updated in PAL","2020-03-30","","Completed","2020-02-16","No","No","No","Internal"]
[null,null,null,null,7884,"98_Thu Sep 12 2019 16:29:07 GMT+0000 (Coordinated Universal Time)","2019-11-18","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Midship port crane hook locking plate missing","Deck - Machinery","Cargo / Ballast Systems","Equipment Related","8.73","Medium","","","Locking plate to be fabricated","2020-03-01","","Completed","2020-01-03","No","No","No","Internal"]
[null,null,null,null,7885,"98_Thu Sep 12 2019 19:53:12 GMT+0000 (Coordinated Universal Time)","2019-11-18","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Bunker Tank Remote Gauges in CCR Showing Erratic Readings","Elect. Mach. & Equip.","General Appearance","Human Error,Inappropriate Procedure","8.23","Medium","","","To be Checked.reactified","2020-01-10","","Completed","2020-01-20","No","No","No","Internal"]
[null,null,null,null,7888,"98_Thu Dec 12 2019 09:11:03 GMT+0000 (Coordinated Universal Time)","2019-11-18","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Pump room davit crane hook locking plate missing","Miscellaneous","General Appearance","Human Error","8.73","Medium","","","Locking plate to be fabricated ","2020-01-30","","Completed","2020-01-03","No","No","No","Internal"]
[null,null,null,null,7889,"98_Thu Dec 12 2019 09:13:46 GMT+0000 (Coordinated Universal Time)","2019-11-18","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Flame screen for vents around accommodation observed to be damaged","Deck - Pipe / Fittings","General Appearance","Human Error","10.8","Medium","","","Damaged flame screens to be renewed","2020-02-15","","Completed","2020-02-12","No","No","No","Internal"]
[null,null,null,null,7890,"98_Thu Dec 12 2019 09:16:06 GMT+0000 (Coordinated Universal Time)","2019-11-18","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Name tags for certain vent.Capacity stencils on certain containment trays around vents missing\n\n","Miscellaneous","General Appearance","Human Error","11.7","High","","","Stenciling to be done","2020-03-20","","Completed","2020-03-12","No","No","No","Internal"]
[null,null,null,null,7891,"98_Thu Dec 12 2019 09:18:11 GMT+0000 (Coordinated Universal Time)","2019-11-18","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","All containment trays to be cleaned from inside","Miscellaneous","MARPOL Related","Human Error","6.9","Low","","","Containment trays to be cleaned","2020-02-15","","Completed","2020-01-24","No","No","No","Internal"]
[null,null,null,null,7892,"98_Thu Dec 12 2019 09:19:48 GMT+0000 (Coordinated Universal Time)","2019-11-18","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","No-2 deck store stbd spare locker securing handle seized","Miscellaneous","General Appearance","Human Error","11.8","Low","","","Door legs to be freed","2020-02-15","","Completed","2020-01-07","No","No","No","Internal"]
[null,null,null,null,7893,"98_Thu Dec 12 2019 09:21:49 GMT+0000 (Coordinated Universal Time)","2019-11-18","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Vent for steering gear on poop deck to be freed","Miscellaneous","General Appearance","Human Error","11.7","High","","","Vents to be freed and greased","2020-02-15","","Completed","2020-01-27","No","No","No","Internal"]
[null,null,null,null,7894,"98_Thu Dec 12 2019 09:23:37 GMT+0000 (Coordinated Universal Time)","2019-11-18","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Paying out direction to be marked on mooring winches","Miscellaneous","General Appearance","Human Error","11.2","Medium","","","Direction to be marked in all winches","2020-03-15","","Completed","2020-03-12","No","No","No","Internal"]
[null,null,null,null,7895,"98_Thu Dec 12 2019 09:26:00 GMT+0000 (Coordinated Universal Time)","2019-11-18","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Flange for IG line drain in the aft leaking","Inert Gas","Cargo / Ballast Systems","Human Error","8.25","Very High","","","leakage to be reactified","2020-02-15","","Completed","2019-12-24","No","No","No","Internal"]
[null,null,null,null,7897,"98_Thu Dec 12 2019 09:31:18 GMT+0000 (Coordinated Universal Time)","2019-11-18","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Soft patch on 2 locations in IG line going to Slop-P & Slop-S","Deck - Pipe / Fittings","Cargo / Ballast Systems","Human Error","8.25","Very High","","","Concerned sections of IG line renewed.","2020-02-15","","Completed","2020-01-03","No","No","No","Internal","This defect noticed in Nov'19, confirm if same rectified. Update DDL accordingly."]
[null,null,null,null,7899,"98_Thu Dec 12 2019 09:38:30 GMT+0000 (Coordinated Universal Time)","2019-11-18","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","3 nos soft patches on VRC line on the hydraulic tank","Cargo Mach.","Cargo / Ballast Systems","Human Error","8.11","Medium","","","VRC return line where soft patch were found renewed.","2020-02-15","","Completed","2020-01-02","No","No","No","Internal"]
[null,null,null,null,7900,"98_Thu Dec 12 2019 09:40:21 GMT+0000 (Coordinated Universal Time)","2019-11-18","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Vacuum pump bulkhead bearing showing tell tale signs for leakage","Cargo Mach.","Cargo / Ballast Systems","Human Error","8.8","Medium","","","To be inspected and reactified","2020-02-15","","Completed","2020-01-08","No","No","No","Internal"]
[null,null,null,null,7901,"98_Thu Dec 12 2019 09:43:32 GMT+0000 (Coordinated Universal Time)","2019-11-18","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Bonding cables for piplines missing / cracked at various locations","Deck - Pipe / Fittings","Cargo / Ballast Systems","Human Error","8.39","Medium","","","Bonding cables to be fixed","2020-05-20","","Completed","2020-04-18","No","No","No","Internal"]
[null,null,null,null,7902,"98_Thu Dec 12 2019 09:45:57 GMT+0000 (Coordinated Universal Time)","2019-11-18","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","COW line dressor leaking on top of No2 COT","Deck - Pipe / Fittings","Cargo / Ballast Systems","Human Error","8.34","High","","","Inspection to be done and leakage to be arrested","2020-02-15","","Completed","2019-12-22","No","No","No","Internal"]
[null,null,null,null,7903,"98_Thu Dec 12 2019 09:53:40 GMT+0000 (Coordinated Universal Time)","2019-11-18","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Excessive play in mooring winch engaging levers","Deck - Machinery","Mooring","Human Error","9.14","Medium","","","Eangaging lever to be readjusted","2020-02-15","","Completed","2020-01-06","No","No","No","Internal"]
[null,null,null,null,7904,"98_Thu Dec 12 2019 13:49:36 GMT+0000 (Coordinated Universal Time)","2019-11-18","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Port & Stbd anchor having twist in cable & not housing completely","Deck - Machinery","Mooring","Human Error","9.14","Medium","","","Twist of the cable to be cleared , so housing completely","2020-02-15","","Completed","2020-01-13","No","No","No","Internal"]
[null,null,null,null,7905,"98_Thu Dec 12 2019 13:51:15 GMT+0000 (Coordinated Universal Time)","2019-11-18","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Rollers on deck to be free’d","Deck - Machinery","Mooring","Human Error","9.14","Medium","","","Rollers to be freed and greased","2020-02-15","","Completed","2020-01-22","No","No","No","Internal"]
[null,null,null,null,7906,"98_Thu Dec 12 2019 13:52:58 GMT+0000 (Coordinated Universal Time)","2019-11-18","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","PV valves to be free’d for movement","Deck - Pipe / Fittings","Cargo / Ballast Systems","Human Error","8.21","High","","","to be freed","2020-02-15","","Completed","2020-01-07","No","No","No","Internal"]
[null,null,null,null,7907,"98_Thu Dec 12 2019 13:55:17 GMT+0000 (Coordinated Universal Time)","2019-11-18","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Soft patch on galley supply vent stbd side B-deck","Miscellaneous","General Appearance","Human Error","11.7","High","","","Soft patch to be removed and permanent repairs to be done","2020-02-15","","Completed","2020-02-14","No","No","No","Internal"]
[null,null,null,null,7908,"98_Thu Dec 12 2019 13:57:32 GMT+0000 (Coordinated Universal Time)","2019-11-18","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Recommend to Shift wilden pump aft of fish plate","Miscellaneous","MARPOL Related","Human Error","6.3","Low","","","Wilden pumps to be shifted to aft of fish plate","2020-02-15","","Completed","2020-01-04","No","No","No","Internal"]
[null,null,null,null,7909,"98_Thu Dec 12 2019 13:59:57 GMT+0000 (Coordinated Universal Time)","2019-11-18","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Tank numbers to be stencilled on COW machines","Miscellaneous","General Appearance","Human Error","11.4","Very High","","","Stenciling / markings to be done","2020-03-15","","Completed","2020-03-12","No","No","No","Internal"]
[null,null,null,null,7910,"98_Thu Dec 12 2019 14:01:50 GMT+0000 (Coordinated Universal Time)","2019-11-18","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Air hose for gangway having superficial cracks","Deck - Machinery","General Appearance","Human Error","11.4","Very High","","","Hose renewed.","2020-05-20","","Completed","2020-04-30","No","No","No","Internal","This defect noticed in Nov'19, confirm if same rectified. Update DDL accordingly."]
[null,null,null,null,7911,"98_Thu Dec 12 2019 14:03:49 GMT+0000 (Coordinated Universal Time)","2019-11-18","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","“Danger lack of oxygen” to be stencilled on cargo tank domes and ballast tank covers","Miscellaneous","General Appearance","Human Error","11.2","Medium","","","Stenciling to be done","2020-03-15","","Completed","2020-03-07","No","No","No","Internal"]
[null,null,null,null,7912,"98_Thu Dec 12 2019 14:05:52 GMT+0000 (Coordinated Universal Time)","2019-11-18","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Shackles and web slings to be have ID’s and inspection to be carried out","Miscellaneous","Cargo / Ballast Systems","Inappropriate Procedure","8.5","Very High","","","To be identified, insected and marking to be done","2020-03-15","","Completed","2020-03-10","No","No","No","Internal"]
[null,null,null,null,7913,"98_Thu Dec 12 2019 14:08:36 GMT+0000 (Coordinated Universal Time)","2019-11-18","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Securing clamps for manifold grating missing and stbd grating bent at one location","Miscellaneous","General Appearance","Inappropriate Procedure","11.3","Medium","","","Securing clamps to be fixed on gratings","2020-01-15","","Completed","2020-01-01","No","No","No","Internal"]
[null,null,null,null,7914,"98_Thu Dec 12 2019 14:22:42 GMT+0000 (Coordinated Universal Time)","2019-11-18","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Anchor wash port valve gland packing leaking","Deck - Pipe / Fittings","General Appearance","Human Error","11.4","Very High","","","Gland packing to be renewed","2020-01-15","","Completed","2020-01-11","No","No","No","Internal"]
[null,null,null,null,7915,"98_Thu Dec 12 2019 14:24:36 GMT+0000 (Coordinated Universal Time)","2019-11-18","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Forward educator overboard valves to be sealed","Deck - Pipe / Fittings","MARPOL Related","Inappropriate Procedure","6.15","High","","","To be sealed","2020-01-10","","Completed","2020-01-04","No","No","No","Internal"]
[null,null,null,null,7916,"98_Thu Dec 12 2019 14:28:35 GMT+0000 (Coordinated Universal Time)","2019-11-18","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Forward ETA drawing to be update name and company","Miscellaneous","General Appearance","Human Error","9.29","Low","","","To be updated","2019-12-25","","Completed","2020-01-26","No","No","No","Internal"]
[null,null,null,null,7917,"98_Thu Dec 12 2019 14:30:34 GMT+0000 (Coordinated Universal Time)","2019-11-18","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Stbd bitter end sledge hammer missing","Miscellaneous","General Appearance","Human Error","9.2","Very High","","","To be placed back in place","2019-12-20","","Completed","2020-01-01","No","No","No","Internal"]
[null,null,null,null,7918,"98_Thu Dec 12 2019 14:32:11 GMT+0000 (Coordinated Universal Time)","2019-11-18","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Step for port windlass operating platform damaged","Deck - Pipe / Fittings","General Appearance","Human Error","11.1","High","","","To be renewed","2019-12-20","","Completed","2019-12-28","No","No","No","Internal"]
[null,null,null,null,7919,"98_Thu Dec 12 2019 14:33:45 GMT+0000 (Coordinated Universal Time)","2019-11-18","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","‘SNAP BACK ZONE’ markings on mooring area missing","Miscellaneous","General Appearance","Inappropriate Procedure","9.26","Low","","","To be marked","2020-03-28","","Completed","2020-03-12","No","No","No","Internal"]
[null,null,null,null,7920,"98_Thu Dec 12 2019 14:37:25 GMT+0000 (Coordinated Universal Time)","2019-11-18","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Edges of containment try around mooring winches wasted / holes at various locations","Deck - Pipe / Fittings","General Appearance","Human Error","6.9","Low","","","repaired","2020-02-28","","Completed","2020-01-14","No","No","No","Internal"]
[null,null,null,null,7921,"98_Thu Dec 12 2019 14:44:32 GMT+0000 (Coordinated Universal Time)","2019-11-18","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Step at the entrance of pump room wasted / holed","Deck - Pipe / Fittings","General Appearance","Human Error","11.1","High","","","repaired","2020-02-15","","Completed","2020-01-08","No","No","No","Internal"]
[null,null,null,null,7922,"98_Thu Dec 12 2019 14:46:13 GMT+0000 (Coordinated Universal Time)","2019-11-18","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Extensive cleaning required in pump room bottom area","Miscellaneous","General Appearance","Human Error","8.44","High","","","cleaned and painted","2020-02-15","","Completed","2019-12-24","No","No","No","Internal"]
[null,null,null,null,7923,"98_Thu Dec 12 2019 14:50:35 GMT+0000 (Coordinated Universal Time)","2019-11-18","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Spare impellers kept in pump room to be properly covered","Miscellaneous","General Appearance","Human Error","11.1","High","","","properly secured","2020-01-10","","Completed","2020-01-03","No","No","No","Internal"]
[null,null,null,null,7924,"98_Thu Dec 12 2019 14:53:34 GMT+0000 (Coordinated Universal Time)","2019-11-18","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Cleaning of oil stains from few light fixtures in pump room","Miscellaneous","General Appearance","Human Error","8.44","High","","","cleaned","2020-01-15","","Completed","2019-12-28","No","No","No","Internal"]
[null,null,null,null,7925,"98_Thu Dec 12 2019 15:03:11 GMT+0000 (Coordinated Universal Time)","2019-11-18","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Protection Shield for grinder has become opaque","Miscellaneous","General Appearance","Human Error","5.5","Low","","","Renewed.","2020-01-10","","Completed","2020-01-02","No","No","No","Internal"]
[null,null,null,null,7926,"98_Thu Dec 12 2019 15:05:01 GMT+0000 (Coordinated Universal Time)","2019-11-18","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Clear derbies & staging material from 4s WBT tank","Hull & Tanks","Cargo / Ballast Systems","Human Error","11.1","High","","","debris cleared","2020-02-28","","Completed","2020-02-05","No","No","No","Internal"]
[null,null,null,null,7928,"98_Thu Dec 12 2019 17:03:19 GMT+0000 (Coordinated Universal Time)","2019-11-18","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Suction hoses for wbt gas detection system were observed to be disconnected at midship area","Deck - Pipe / Fittings","General Appearance","Human Error","11.4","Very High","","","lines secured, lines not in use","2020-02-28","","Completed","2020-01-08","No","No","No","Internal"]
[null,null,null,null,7929,"98_Thu Dec 12 2019 17:05:12 GMT+0000 (Coordinated Universal Time)","2019-11-18","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Ballast tank gauge 1s not operational","Deck - Pipe / Fittings","Cargo / Ballast Systems","Human Error","8.22","Very High","","","reactified","2020-01-15","","Completed","2020-01-14","No","No","No","Internal"]
[null,null,null,null,7930,"98_Thu Dec 12 2019 17:07:03 GMT+0000 (Coordinated Universal Time)","2019-11-18","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","COP emergency stop in CCR not operational","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.2","Medium","","","simulated and found in good condition","2020-03-15","","Completed","2020-02-12","No","No","No","Internal"]
[null,null,null,null,7931,"98_Thu Dec 12 2019 17:31:40 GMT+0000 (Coordinated Universal Time)","2019-11-18","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Remote level reading for ROT in CCR showing incorrect reading","Miscellaneous","Cargo / Ballast Systems","Equipment Related","8.22","Very High","","","reactified","2020-02-15","","Completed","2019-12-17","No","No","No","Internal"]
[null,null,null,null,7932,"98_Thu Dec 12 2019 18:30:18 GMT+0000 (Coordinated Universal Time)","2019-11-18","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Front panel for Drawer below bed damaged at 1 location each in 2 cabins ( worker cabin,3rd off)","Accommodation","MLC Related","Human Error","11.8","Low","","","repaired","2019-12-20","","Completed","2019-12-14","No","No","No","Internal"]
[null,null,null,null,8743,"98_16/12/2019 8:20:42 PM","2019-11-22","Breakdown","Ship Staff","Ship Staff Insp.","Soft patch on stripper pump discharge line and air chamber","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.8","Medium","","","Repaired","2019-12-20","","Completed","2020-12-20","No","No","No","Internal"]
[null,null,null,null,7879,"98_Mon Aug 12 2019 17:55:53 GMT+0000 (Coordinated Universal Time)","2019-12-03","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Insulation missing most of the pipe lines","E/R - Aux. Mach.,Miscellaneous","Eng. / Strg. Comp.","Equipment Related,Human Error,Inappropriate Procedure","11.5","Medium","","","Insulation installed.","2020-02-29","","Completed","2020-02-15","No","No","No","Internal"]
[null,null,null,null,8751,"98_23/12/2019 2:49:10 PM","2019-12-04","Defect","FSC Inspector","Flag State Insp.","Sector of stern light incorrect","Navigation - Others","Navigation","Equipment Related","4.8","Medium","","","New stern light fitted with correct sector.","2019-12-07","","Completed","2019-12-07","No","No","No","External"]
[null,null,null,null,8752,"98_23/12/2019 2:53:41 PM","2019-12-04","Defect","FSC Inspector","Flag State Insp.","No.6 Foam Monitor Leaking","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.38","High","","","Valve of Foam Monitor No.6 renewed","2019-12-07","","Completed","2019-12-07","No","No","No","External"]
[null,null,null,null,8753,"98_23/12/2019 3:15:50 PM","2019-12-04","Non Conformity","Owner / Marine / Tech. Suptd.","ISM Audit","Open type transformers found being used in laundry rooms.","Elect. Mach. & Equip.,Miscellaneous","ISM Related","Human Error","","","","","New laundry equipment of 220V fitted.","2019-12-10","","Completed","2019-12-10","No","No","No","Internal"]
[null,null,null,null,8754,"98_23/12/2019 3:58:39 PM","2019-12-04","Defect","Owner / Marine / Tech. Suptd.","ISM Audit","Old managers posters were found posted in crew smoke room and B deck alleyway.","Miscellaneous","ISM Related","Human Error","","","","","Inspection of all common spaces done. All posters from previous management removed.","2019-12-15","","Completed","2019-12-15","No","No","No","Internal"]
[null,null,null,null,8755,"98_23/12/2019 4:03:09 PM","2019-12-04","Defect","Owner / Marine / Tech. Suptd.","MLC Audit","A deck common toilet slope found defective. Stagnant water was found on the floor. ","Accommodation","General Appearance","Human Error","11.13","Low","","","Slope corrected and new tiles fitted in A deck common toilet.","2019-12-07","","Completed","2019-12-07","No","No","No","Internal"]
[null,null,null,null,8742,"98_Wed Dec 11 2019 17:13:10 GMT+0000 (Coordinated Universal Time)","2019-12-05","Defect","Ship Staff","Suptd. Insp.","Control air bottle drain  is plugged","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","Drain valve to be fitted,but this air bottle supplying air to QCV in fire station and if we installed drain valve and opeate the drain valve then bottle pressure will drop and all the QCV will operate.Job has been discarded.","2020-01-31","","Completed","2019-12-31","No","No","No","Internal"]
[null,null,null,null,7887,"98_Tue Nov 12 2019 17:13:10 GMT+0000 (Coordinated Universal Time)","2019-12-05","Defect","Ship Staff","Suptd. Insp.","Control air bottle drain  is plugged","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","As per original design drain plug is not fitted. Safety Equipment.","2020-01-31","","Completed","2020-05-31","No","No","No","Internal","This defect is very old, pls update if same rectified."]
[null,null,null,null,7936,"98_Thu Dec 12 2019 18:59:56 GMT+0000 (Coordinated Universal Time)","2019-12-18","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Stencil “ventilate prior entering” at lifeboat entrance","LSA / FFA","Safety / LSA / FFA","Human Error","5.27","Medium","","","stenciled","2019-12-20","","Completed","2020-01-03","No","No","No","Internal"]
[null,null,null,null,7939,"98_Thu Dec 12 2019 19:07:13 GMT+0000 (Coordinated Universal Time)","2019-12-18","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Inspection tags for EEBD / Extinguishers to be updated","LSA / FFA","Safety / LSA / FFA","Human Error","5.27","Medium","","","All tags  changed","2019-12-20","","Completed","2020-01-04","No","No","No","Internal"]
[null,null,null,null,7940,"98_Thu Dec 12 2019 19:09:48 GMT+0000 (Coordinated Universal Time)","2019-12-18","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Inventory of helicopter gear to be taken and updated","LSA / FFA","Safety / LSA / FFA","Human Error","5.13","High","","","inventory to be updated","2019-12-20","","Completed","2020-01-06","No","No","No","Internal"]
[null,null,null,null,7896,"98_Thu Dec 12 2019 09:28:10 GMT+0000 (Coordinated Universal Time)","2019-12-18","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Ship side railing broken and bent at various location,Railings on top of midship locker bent\n\n","Deck - Pipe / Fittings","General Appearance","Human Error","11.5","Medium","","","Railings renewed","2020-02-15","","Completed","2020-01-12","No","No","No","Internal"]
[null,null,null,null,7933,"98_Thu Dec 12 2019 18:32:55 GMT+0000 (Coordinated Universal Time)","2019-12-18","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Rubber packing for port side bridge wing door damaged","Accommodation","General Appearance","Human Error","11.6","Medium","","","repaired","2020-02-28","","Completed","2020-02-20","No","No","No","Internal"]
[null,null,null,null,7934,"98_Thu Dec 12 2019 18:44:16 GMT+0000 (Coordinated Universal Time)","2019-12-18","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Replace Fire plan IMO symbol with burning ship","LSA / FFA","Safety / LSA / FFA","Human Error","","","","","imo symbol replaced","2020-02-20","","Completed","2020-02-20","No","No","No","Internal"]
[null,null,null,null,7935,"98_Thu Dec 12 2019 18:55:58 GMT+0000 (Coordinated Universal Time)","2019-12-18","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Embarkation ladders for forward life rafts and both lifeboats to be inspected","LSA / FFA","Safety / LSA / FFA","Human Error","5.27","Medium","","","ladders inspected. Fwd liferaft ladder replaced with new one.","2019-12-20","","Completed","2020-01-03","No","No","No","Internal"]
[null,null,null,null,null,"98_30/4/2020 6:51:22 PM","2020-01-01","Defect","Ship Staff","Ship Staff Insp.","DECK SEAL PUMP#2","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related,External Factors,Human Error",10.32,"Very High","Not Applicable","Not Applicable","PUMP FRAME ARE IN CORRODED CONDITION,SHAFT WORN OUT STATE.PUMP IS IN RUNNING CONDITION BUT LOW FLOW RATE","2020-07-30","RO200017","Completed","2020-07-23","No",null,null,"Internal"]
[null,null,null,null,null,"98_15/7/2020 10:47:10 PM","2020-01-01","Defect","Ship Staff","Ship Staff Insp.","Inert Gas Blower#1 ","Cargo Mach.,E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related,External Factors,Human Error",8.17,"Low","Not Applicable","Not Applicable","Kindly note, vessel noticed during running of IG Blower #1 heavily vibrating on the base to surrounding periphery. Fwd And Aft Bearing Temperature reading are 20°C more higher than as compared to IG Blower # 2.(IG Blower#1 Readings: Bearing:84 Deg C and Aft Bearing:77 Deg C).\r\n\r\n Blower are running with 20-25 Amps lower than IG Blower #2 (IG Blower #1:50A,IG Blower # 2:72A)\r\n\r\nIn addition the slight amount of gas Leaking from blower Carbon seal ring due to wear down of seal IMPELLER RECEIVED AFTER RECONDITIONING, IMPELLER INSTALLED AND IG BLOWER NO. 1 TRIED OUT, PERFORMANCE SATISFACTORY.\r\n","2020-07-20","PO200130,off-landed in singapore for on 11.07.2020 for repair and balancing","Completed","2020-07-24","No",null,null,"Internal"]
[null,null,null,null,null,"98_6/7/2020 12:01:04 AM","2020-01-03","Breakdown,Defect","Ship Staff","Ship Staff Insp.","MAIN ENGINE VISCOSITY CONTROL UNIT","E/R - Main Engine,Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related,External Factors,Human Error,Inappropriate Procedure",10.32,"Very High","Not Applicable","Not Applicable","PUMP OUT OF OPERATION,TEMPERATUR OPERATING BY MANUALLY","2020-07-31","RO200036","Completed","2020-07-28","No",null,null,"Internal"]
[null,null,null,null,null,"98_6/7/2020 12:02:34 AM","2020-01-03","Breakdown,Defect","Ship Staff","Ship Staff Insp.","AUXILIARY ENGINE VISCOSITY CONTROL UNIT","E/R - Aux. Engine,Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related,External Factors,Human Error,Inappropriate Procedure",10.32,"Very High","Not Applicable","Not Applicable","System tried out after changing over to VLSFO, observed working in temperature control mode, but not working in viscosity control mode, same needs to be further troubleshooted.","2020-08-15","RO200036","Completed","2020-07-28","No",null,null,"Internal"]
[null,null,null,null,12169,"98_9/4/2020 9:12:16 AM","2020-02-04","Observation","Owner / Marine / Tech. Suptd.","Bunkering Audit","Bunker transfer plan / checklist 12.04.08.011.01 section 7 - monitoring of H2S/Benzene vapors : Benzene reading measured by detector tubes shall be mentioned < Min value that can be measurd by the specific tube.\n\nFor example by gastec tubes min measurable value is 0.05 ppm, hence in that case benzene shall be mentioned <0.05ppm(if no discoloration observed) Understand vessel has kept the gas tube as evidence of monitoring.\n\n","Documentation","ISM Related","Human Error,Inappropriate Procedure","","","","","Corrective Action:All the previous Oil Transferring plan/ Checklist 12.04.08.011.02 section 7- the value are corrected < Min value which is for H2S is < 0.2 and for Benzene < 0.1 as per gastec tubes min reading.\n\n\n\nVessel has kept previous all bunkering gastec tubes as evidence of monitoring.\n\n\n\nPreventive Action: Briefed all Engineers and officers for correct measuring method of the gastec tube reading in future bunkering and cargo operation.\n\n\n\n","2020-04-10","","Completed","2020-04-10","No","No","No","Internal"]
[null,null,null,null,null,"98_27/6/2020 10:33:50 AM","2020-02-17","Critical Equipment,Defect","Ship Staff","Ship Staff Insp.","ENGINE ROOM HIGH EXPANSION FOAM SYSTEM","LSA / FFA","Safety / LSA / FFA","Behaviour Based,Equipment Related,External Factors,Inappropriate Procedure",5.4,"High","Not Applicable","Not Applicable","FOAM TANK PROPOTIONAL VALVE DIAPHRAGM CHANGED WITH NEW SPARE RECIEVED AND SYSTEM MADE OPERATIONAL.","2020-07-31","RO200094","Completed","2020-07-22","No",null,null,"Internal"]
[null,null,null,null,12170,"98_2/3/2020 1:19:59 AM","2020-03-01","Defect","Ship Staff","Ship Staff Insp.","ME LO Plate Cooler","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related,Human Error","10.32","Very High","","","All the Sea Water and Lub oil Side Plate cleaned.","2020-04-15","PO205007","Completed","2020-04-04","No","No","No","Internal"]
[null,null,null,null,null,"98_2/3/2020 1:22:40 AM","2020-03-01","Defect","Ship Staff","Ship Staff Insp.","MAIN ENGINE CROSSHEAD PUMP#1","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related,Human Error",10.32,"Very High","Not Applicable","Not Applicable","Pump are overhauled by shore tech.","2020-07-31","RO200068","Completed","2020-07-12","No",null,null,"Internal"]
[null,null,null,null,null,"98_2/3/2020 1:25:58 AM","2020-03-01","Defect","Ship Staff","Ship Staff Insp.","MAIN ENGINE LUBRICATING DEVICE","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related,Human Error",10.32,"Very High","Not Applicable","Not Applicable","3 Pcs of Element Leaking for Oil,At Present the Lekages has been partially arrested with teflon and unit are in woring state.","2020-07-31","RO200107 & RO200244","Completed","2020-07-15","No",null,null,"Internal"]
[null,null,null,null,null,"98_30/4/2020 6:25:47 PM","2020-03-10","Defect,Observation","Ship Staff","Ship Staff Insp.","PROVISION CRANE 2.5 TONS","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related,Human Error,Inappropriate Procedure",8.73,"Medium","Not Applicable","Not Applicable","REMOTE BUTTONS IS BRITTLE AND BROKEN,RECEPTACLE AND PLUG ARE IN CORRODED AND BROKEN  DUE TO AEGING.SPARES RECEIVED IN CHINA AND FOUND SATISFACTORY.","2020-07-30","RO200174","Completed","2020-06-15","No",null,null,"Internal"]
[null,null,null,null,12171,"98_15/3/2020 4:30:41 PM","2020-03-14","Defect,Observation","Ship Staff","Ship Staff Insp.","Provision crane 0.9 Tons","Elect. Mach. & Equip.,Hull & Tanks","General Appearance","Equipment Related,Human Error,Inappropriate Procedure","8.73","Medium","","","Crane Limit switch securing bracket to be fabricated.","2020-04-30","","Completed","2020-04-13","No","No","No","Internal"]
[null,null,null,null,12172,"98_15/3/2020 4:27:52 PM","2020-03-15","Defect","Ship Staff","Ship Staff Insp.","Aft Poop Deck and Em generator Fire sea water line","Critical Equip.,Deck - Pipe / Fittings,LSA / FFA","Safety / LSA / FFA","Equipment Related,Human Error","5.35","Medium","","","2 pcs of section of the fire line to be renewed.","2020-05-30","","Completed","2020-05-15","No","No","No","Internal"]
[null,null,null,null,null,"98_27/3/2020 3:29:50 PM","2020-03-16","Observation","Ship Staff","Ship Staff Insp.","VECS System O2 sensor expired May' 17.","Inert Gas","Cargo / Ballast Systems","Equipment Related",8.17,"Low","Not Applicable","Not Applicable","RO Raised for new sensor.","2020-07-15","RO200139","Completed","2020-07-15","No",null,null,"Internal"]
[null,null,null,null,null,"98_30/4/2020 6:32:09 PM","2020-03-26","Defect,Observation","Ship Staff","Ship Staff Insp.","MAIN ENGINE LOCAL MANEUVERING STAND PRESSURE GAUGES","E/R - Main Engine,Miscellaneous","Eng. / Strg. Comp.","Equipment Related,External Factors,Human Error",6.8,"High","Not Applicable","Not Applicable","3 Pcs of Local Pressure Gauges  glass replaced with new spare received.","2020-07-30","RO200157","Completed","2020-08-05","No",null,null,"Internal"]
[null,null,null,null,null,"98_30/4/2020 6:29:31 PM","2020-04-04","Defect,Observation","Ship Staff","Ship Staff Insp.","AUX BOILER ECO FEED WATER PUMP SPARES","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related,External Factors",10.32,"Very High","Not Applicable","Not Applicable","Pump casing renewed.","2020-07-30","RO200038","Completed","2020-07-20","No",null,null,"Internal"]
[null,null,null,null,null,"98_29/4/2020 10:55:06 AM","2020-04-20","Defect,Observation","Ship Staff","Ship Staff Insp.","BACK UP BALLAST PUMP","Elect. Mach. & Equip.","Cargo / Ballast Systems","Equipment Related,Human Error",10.32,"Very High","Not Applicable","Not Applicable","Back Up Ballast Pump RTD Transducer and Safety Barrier are not in operational state.Pump is in Operational State.","2020-07-30","RO200182","Completed","2020-07-16","No",null,null,"Internal"]
[null,null,null,null,null,"98_29/4/2020 10:52:12 AM","2020-04-23","Defect","Ship Staff","Ship Staff Insp.","ME SHAFT EARTHING DEVICE","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related,Human Error",10.32,"Very High","Not Applicable","Not Applicable","SILVER ALLOY BAND WORN OUT,NEED TO RENEWED THE BAND,INSTRUMENT IS IN OPERATIONAL CONDITION","2020-07-30","RO200192","Completed","2020-07-16","No",null,null,"Internal"]
[null,null,null,null,null,"98_30/4/2020 6:36:50 PM","2020-04-30","Defect","Ship Staff","Ship Staff Insp.","FRESH WATER GENERATOR","E/R - Aux. Mach.,Miscellaneous","Eng. / Strg. Comp.","Equipment Related,External Factors,Human Error,Inappropriate Procedure",10.32,"Very High","Not Applicable","Not Applicable","FLOWMETER AND NRV CHANGED WITH NEW SPARE. FEED LINE REPLACED WITH NEW FABRICATED SECTION WITH NEW UNIONS AND CONNECTIONS","2020-07-30","RO200199","Completed","2020-07-21","No",null,null,"Internal"]
[null,null,null,null,12670,"98_13/6/2020 7:13:27 AM","2020-05-05","Observation","Ship Staff","Ship Staff Insp.","life buoy light holder securing to ship side railing found worn out","LSA / FFA","Safety / LSA / FFA","Human Error","5.31","High","","","Holder to be renewed","2020-05-10","","Completed","2020-05-09","No","No","No","Internal"]
[null,null,null,null,12671,"98_13/6/2020 6:26:21 AM","2020-05-08","Observation","Ship Staff","Ship Staff Insp.","Engine room- bottom platform portable extinguisher securing straps broken.","LSA / FFA","Eng. / Strg. Comp.","Equipment Related,Human Error","5.35","Medium","","","securing  strap to be renewed","2020-05-15","","Completed","2020-05-10","No","No","No","Internal"]
[null,null,null,null,12672,"98_13/6/2020 7:17:48 AM","2020-05-08","Observation","Ship Staff","Ship Staff Insp.","Ship side railing found heavly corroded and bent at certain locations","Deck - Pipe / Fittings","General Appearance","External Factors,Human Error","11.1","High","","","To be de rusted and streightened","2020-05-30","","Completed","2020-05-21","No","No","No","Internal"]
[null,null,null,null,12673,"98_13/6/2020 7:41:12 AM","2020-05-08","Defect","Ship Staff","Ship Staff Insp.","Lifeboat bilge pump discharge hose section wasted","LSA / FFA","Safety / LSA / FFA","Equipment Related,Human Error","5.29","High","","","Hose to be renewed","2020-05-10","","Completed","2020-05-09","No","No","No","Internal"]
[null,null,null,null,12674,"98_14/6/2020 1:15:04 PM","2020-05-09","Observation","Ship Staff","Ship Staff Insp.","STEERING GEAR ROOM ","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related,External Factors,Human Error","10.32","Very High","","","STEERING GEAR ROOM AUTO DRAIN VALVE SEIZED.","2020-05-15","","Completed","2020-05-10","No","No","No","Internal"]
[null,null,null,null,12675,"98_13/6/2020 7:20:59 AM","2020-05-12","Breakdown","Ship Staff","Ship Staff Insp.","Bunker line on deck with spot pitting and small hole near pump room entrance","Deck - Pipe / Fittings","General Appearance","External Factors,Human Error","2.16","Medium","","","Pipe line to be renewed","2020-05-15","","Completed","2020-05-14","No","No","No","Internal"]
[null,null,null,null,12676,"98_13/6/2020 7:02:02 AM","2020-05-15","Non Conformity","Ship Staff","Ship Staff Insp.","Deck Safety walkway gratings heavly corroded","Deck - Pipe / Fittings","General Appearance","Human Error","11.1","High","","","To be renewed","2020-05-25","","Completed","2020-05-18","No","No","No","Internal"]
[null,null,null,null,12677,"98_14/6/2020 1:19:45 PM","2020-05-16","Critical Equipment,Non Conformity,Observation","Ship Staff","Ship Staff Insp.","ENGINE ROOM FUNNEL FLAPS","Critical Equip.,Miscellaneous","Eng. / Strg. Comp.","Equipment Related,External Factors,Human Error,Inappropriate Procedure","5.35","Medium","","","REMOTE OPERATING HANDLE FOUND IN CORRODED CONDITION.","2020-05-18","","Completed","2020-05-16","No","No","No","Internal"]
[null,null,null,null,null,"98_20/5/2020 11:13:28 AM","2020-05-16","Defect,Observation","Ship Staff","Ship Staff Insp.","AFT POOP DECK STBD MOORING WINCH","Deck - Mooring Machinery","Mooring","Equipment Related,Human Error,Inappropriate Procedure",9.14,"Medium","Not Applicable","Not Applicable","seal changed and leak rectified.","2020-07-30","RO200221","Completed","2020-08-18","No",null,null,"Internal"]
[null,null,null,null,null,"98_20/5/2020 10:56:56 AM","2020-05-20","Defect","Ship Staff","Ship Staff Insp.","PROVISION CRANE 2.5 TONS","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related,Inappropriate Procedure",8.73,"Medium","Not Applicable","Not Applicable","Hoisting Motor Pedestal Bearing Cover and bearing changed with new spare received, system operational","2020-07-30","RO200224","Completed","2020-07-31","No",null,null,"Internal"]
[null,null,null,null,null,"98_23/5/2020 11:11:06 AM","2020-05-20","Defect","Ship Staff","Ship Staff Insp.","ME LUB OIL PURIFIER","E/R - Purifier","Eng. / Strg. Comp.","Equipment Related,External Factors",10.32,"Very High","Not Applicable","Not Applicable","PCB REPLACED WITH NEW SPARE RECEIVED, SYSTEM OPERATIONAL.","2020-07-30","RO200225","Completed","2020-07-29","No",null,null,"Internal"]
[null,null,null,null,null,"98_27/5/2020 3:00:14 PM","2020-05-25","Defect","Ship Staff","Ship Staff Insp.","FRESH WATER GENERATOR","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related,Inappropriate Procedure",10.32,"Very High","Not Applicable","Not Applicable","FLOW METER CHANGED WITH NEW","2020-07-30","RO200233","Completed","2020-07-21","No",null,null,"Internal"]
[null,null,null,null,null,"98_7/6/2020 7:33:27 PM","2020-06-02","Breakdown,Defect","Ship Staff","Ship Staff Insp.","FE AND CU IONS GENERATING UNITS","E/R - Aux. Mach.,E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related,Inappropriate Procedure",10.32,"Very High","Not Applicable","Not Applicable","ALL THE ANODES RENEWED.","2020-07-30","RO200032","Completed","2020-07-13","No",null,null,"Internal"]
[null,null,null,null,null,"98_14/6/2020 1:11:14 PM","2020-06-14","Defect","Ship Staff","Ship Staff Insp.","S-BAND RADAR","Elect. Mach. & Equip.,Navigation - RADAR","Navigation","Equipment Related,External Factors,Human Error,Inappropriate Procedure",4.7,"High","Not Applicable","Not Applicable","PCB MALFUNCTIOING,At present no alarm display PCB Renewed.","2020-07-20","RO200242","Completed","2020-07-13","No",null,null,"Internal"]
[null,null,null,null,12826,"98_22/6/2020 5:28:46 AM","2020-06-21","Defect,Non Conformity","Ship Staff","Ship Staff Insp.","Air vent float of fore peak tank found in damaged codition","Deck - Pipe / Fittings","Cargo / Ballast Systems","External Factors","11.7","High","","","Flaot renewed","2020-06-25","","Completed","2020-06-21","No","No","No","Internal"]
[null,null,null,null,12827,"98_29/6/2020 9:29:49 AM","2020-06-26","Observation","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","The insulation meter on switchboard for accommodation (220-volt system) showed 1.0megohm, it was back to normal during inspection.","Elect. Mach. & Equip.","ISM Related","Human Error","10.38","Medium","","","Electrical equipment was connected to power point by third party. It was removed.","2020-06-27","","Completed","2020-06-26","No","No","No","External"]
[null,null,null,null,null,"98_29/6/2020 9:37:05 AM","2020-06-26","Observation","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","Marine growth about 30% of the visible area (under summer draft) was found on ship’s hull.","Hull & Tanks","General Appearance","External Factors",11.1,"High","Not Applicable","Not Applicable","Hull cleaning carried out.","2020-07-20",null,"Completed","2020-07-15","No",null,null,"External"]
[null,null,null,null,null,"98_29/6/2020 9:45:12 AM","2020-06-26","Observation","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","Noted maintenance was in progress, some sections of hydraulic pipes (about 10% of area) near COT 4C (about 30m) was moderately rusted.","Deck - Pipe / Fittings","General Appearance","External Factors",11.4,"Very High","Not Applicable","Not Applicable","De-rusting of concerned section to be carried out. Renewal of sections if necessary.","2020-07-31","AZIM200214","Completed","2020-10-31","No",null,null,"External"]
[null,null,null,null,null,"98_4/7/2020 10:36:07 AM","2020-07-02","Breakdown,Defect","Ship Staff","Ship Staff Insp.","VACUUM CONDENSER LEVEL CONTROL VALVE","Cargo Mach.,E/R - Aux. Mach.","Eng. / Strg. Comp.","Behaviour Based,Equipment Related,Human Error,Inappropriate Procedure",10.32,"Very High","Not Applicable","Not Applicable","New 3-way valve installed ","2020-07-31","RO200249","Completed","2020-12-21","No",null,null,"Internal"]
[null,null,null,null,null,"98_15/8/2020 9:04:14 PM","2020-07-21","Defect","Ship Staff","Ship Staff Insp.","Observed Eco Feed Pump no.1 drawing high current after renewal of pump casing. Shaft out of alignment.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related",null,null,"Not Applicable","Not Applicable","Spares received at Fujairah on 26 Oct 2020. Repairs carried out on Eco Feed Pump no.1, pump tried out, performance satisfactory.","2020-09-25","AMAL 200273","Completed","2020-10-29","No",null,null,"Internal"]
[null,null,null,null,null,"98_12/8/2020 1:24:15 PM","2020-08-07","Defect","Ship Staff","Ship Staff Insp.","safety system of ME is not working because of PCB is getting hang frequently","E/R - Main Engine,Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related",null,null,"Not Applicable","Not Applicable","PCB cards received, spare replaced by shore technician from NICO. System working satisfactorily.","2020-09-26","AZIM205081","Completed","2020-10-26","No",null,null,"Internal"]
[null,null,null,null,null,"98_17/9/2020 5:09:49 AM","2020-09-11","Defect","Ship Staff","Ship Staff Insp.","Galley AC blower fins damaged","Accommodation","General Appearance","Equipment Related",null,null,"Not Applicable","Not Applicable","Galley AC Blower spare received on 26 Oct 2020, spare Blower fitted in Galley AC, tried out, performance satisfactory.","2020-10-11","AZIM200296","Completed","2020-11-04","No",null,null,"Internal"]
[null,null,null,null,null,"98_4/11/2020 11:31:38 AM","2020-09-17","Breakdown","Ship Staff","Ship Staff Insp.","1 of the Personnel gas meter & 1 Multi gas meter ( GX-8000) found not working during Monthly Calibration.","Miscellaneous","Cargo / Ballast Systems","Equipment Related",null,null,"Not Applicable","Not Applicable","Awaiting Class Annuals for Repairs and calibration","2020-12-16",null,"Completed","2020-12-16","No",null,null,"Internal"]
[null,null,null,null,null,"98_9/11/2020 11:41:51 AM","2020-10-01","Breakdown,Defect","Ship Staff","Ship Staff Insp.","IG ISOLATION VALVE ON DECK WAS FOUND STUCK IN OPEN POSITION.","Critical Equip.,Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related",null,null,"Not Applicable","Not Applicable","IG VALVE RENEWED","2020-10-29",null,"Completed","2020-10-08","No",null,null,"Internal"]
[null,null,null,null,null,"98_4/11/2020 11:28:13 AM","2020-10-19","Breakdown","Ship Staff","Ship Staff Insp.","VRCS Pressure line near 5P was found leaking","Critical Equip.,Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related",null,null,"Not Applicable","Not Applicable","VRCS pressure line was Renewed","2020-10-24",null,"Completed","2020-10-20","No",null,null,"Internal"]
[null,null,null,null,null,"98_4/11/2020 11:22:27 AM","2020-10-29","Critical Equipment","Ship Staff","Ship Staff Insp.","Deck Machinery - Hyd return lines (2no.s) were found leaking","Deck - Machinery,Deck - Mooring Machinery","Mooring","Equipment Related",null,null,"Not Applicable","Not Applicable","Both the lines were Renewed.","2020-11-01",null,"Completed","2020-11-01","No",null,null,"Internal"]
[null,null,null,null,null,"98_15/11/2020 11:19:36 AM","2020-11-08","Breakdown","Ship Staff","Ship Staff Insp.","Found hole in Fire Pump no. 1 outlet pipe section and water leaking. Pipe section found corroded and wasted. ","E/R - Pipes/ valves & fittings,E/R - Pumps","Eng. / Strg. Comp.","Equipment Related",null,null,"Not Applicable","Not Applicable","Observed water leaking from Fire Pump no. 1 outlet pipe section. Pipe removed from place and new pipe section fabricated in ER Workshop and fitted back in place, no leaks found.","2020-11-11",null,"Completed","2020-11-11","No",null,null,"Internal"]
[null,null,null,null,null,"98_23/11/2020 1:56:37 PM","2020-11-18","Breakdown","Ship Staff","Ship Staff Insp.","Deck Air Compressor abnormal stop and 440V low insulation alarm.Found burning smell coming from Deck Air Compressor radiator cooling fan motor.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related",null,null,"Not Applicable","Not Applicable","New motor boxed back, compressor tried out and working satisfactory.","2020-11-30","AZIM200346","Completed","2020-12-18","No",null,null,"Internal"]

{"sheet":"Calc","index":2,"n_rows":28,"n_cols":12,"rows_kept":28,"cut":false,"hidden":true,"merged":[]}
["Def_type","Def_cause","Equipments","VIQrefno","Observer_code"]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,"Dim itemSele As Long"]
[null,null,null,null,null,null,null,null,null,null,null,"   dim startRow as integer"]
[null,null,null,null,null,null,null,null,null,null,null,"   startRow=1"]
[null,null,null,null,null,null,null,null,null,null,null,"        For itemSele = 0 To ListBox1.ListCount - 1"]
[null,null,null,null,null,null,null,null,null,null,null,"        If ListBox1.Selected(itemSele) = True Then"]
[null,null,null,null,null,null,null,null,null,null,null,"        Worksheets(\"WorksheetName\").Range(\"A\" & startRow).Value = ListBox1.List(itemSele)"]
[null,null,null,null,null,null,null,null,null,null,null,"        startRow = startRow + 1"]
[null,null,null,null,null,null,null,null,null,null,null,"        End If"]
[null,null,null,null,null,null,null,null,null,null,null,"        Next"]
[null,null,null,null,null,null,null,null,null,null,null,"Dim LastRowA As String"]
[null,null,null,null,null,null,null,null,null,null,null,"        Dim itemSele As Long"]
[null,null,null,null,null,null,null,null,null,null,null,"       Dim startRow as integer"]
[null,null,null,null,null,null,null,null,null,null,null,"        LastRowA = ActiveSheet.Cells(Rows.count, \"A\").End(xlUp).row"]
[null,null,null,null,null,null,null,null,null,null,null,"        startQue = 0"]
[null,null,null,null,null,null,null,null,null,null,null,"        For itemSele = 0 To ListBox1.ListCount - 1"]
[null,null,null,null,null,null,null,null,null,null,null,"        For startRow = 1 To LastRowA"]
[null,null,null,null,null,null,null,null,null,null,null,"        If Worksheets(\"WorksheetName\").Range(\"A\" & startRow).Value = ListBox1.List(itemSele) Then"]
[null,null,null,null,null,null,null,null,null,null,null,"        ListBox1.Selected(itemSele) = True"]
[null,null,null,null,null,null,null,null,null,null,null,"        Exit For"]
[null,null,null,null,null,null,null,null,null,null,null,"        End If"]
[null,null,null,null,null,null,null,null,null,null,null,"        Next j"]
[null,null,null,null,null,null,null,null,null,null,null,"        Next"]
[null,null,null,null,null,null,null,null,null,null,null,"        End If"]

{"sheet":"Areaofobs","index":3,"n_rows":17,"n_cols":2,"rows_kept":17,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Cargo / Ballast Systems",11]
["Cert. & Docu.",2]
["Communication",6]
["Crew Management",3]
["Emgcy. Systems",13]
["Eng. / Strg. Comp.",14]
["General Appearance",15]
["Ice Opns.",17]
["ISM Related",7]
["ISPS Related",10]
["MARPOL Related",9]
["MLC Related",4]
["Mooring",12]
["Navigation",5]
["Safety / LSA / FFA",8]
["Structural Condn. / WT integrity ",16]

{"sheet":"Vessel_type","index":4,"n_rows":1,"n_cols":2,"rows_kept":1,"cut":false,"hidden":true,"merged":[]}
["Vessel_type","ID"]

{"sheet":"Deficiency_type","index":5,"n_rows":8,"n_cols":3,"rows_kept":8,"cut":false,"hidden":true,"merged":[]}
["TITLE","Type of deficiency_description","ID"]
["Breakdown",null,6]
["Critical Equipment",null,4]
["Defect",null,1]
["Guarantee Claim",null,8]
["Non Conformity",null,2]
["Observation",null,3]
["Other",null,7]

{"sheet":"VIQrefno","index":6,"n_rows":427,"n_cols":3,"rows_kept":427,"cut":false,"hidden":true,"merged":[]}
["VIQ_ref_no","Risk Value of observation","ID"]
["1.1","Low",8243]
["1.10","Low",8252]
["1.11","Low",8253]
["1.12","Low",8254]
["1.13","Low",8255]
["1.14","Low",8256]
["1.15","Low",8257]
["1.16","Low",8259]
["1.17","Low",8260]
["1.18","Low",8261]
["1.19","Low",8262]
["1.2","Low",8244]
["1.20","Low",8263]
["1.21","Low",8265]
["1.22","Low",8266]
["1.23","Low",8267]
["1.24","Low",8268]
["1.25","Low",8269]
["1.26","Low",8270]
["1.3","Low",8245]
["1.4","Low",8246]
["1.5","Low",8247]
["1.6","Low",8248]
["1.7","Low",8249]
["1.8","Low",8250]
["1.9","Low",8251]
["1.99","High",11258]
["10.1","Medium",8461]
["10.10","High",8470]
["10.11","Medium",8471]
["10.12","Very High",8472]
["10.13","Very High",8473]
["10.14","Medium",8474]
["10.15","Low",8475]
["10.16","Very High",8476]
["10.17","Very High",8477]
["10.18","High",8478]
["10.19","Very High",8479]
["10.2","Low",8462]
["10.20","High",8480]
["10.21","Medium",8481]
["10.22","Low",8482]
["10.23","Medium",8483]
["10.24","Low",8484]
["10.25","Very High",8485]
["10.26","High",8486]
["10.27","Medium",8487]
["10.28","Low",8488]
["10.29","Medium",8489]
["10.3","Medium",8463]
["10.30","High",8490]
["10.31","Very High",8491]
["10.32","Very High",8492]
["10.33","High",8493]
["10.34","High",8494]
["10.35","Very High",8495]
["10.36","Very High",8496]
["10.37","Medium",8497]
["10.38","Medium",8498]
["10.39","High",8499]
["10.4","High",8464]
["10.40","Medium",8500]
["10.41","Medium",8501]
["10.42","Medium",8502]
["10.43","Medium",8503]
["10.44","Medium",8504]
["10.45","Very High",8505]
["10.46","High",8506]
["10.47","Medium",8507]
["10.48","High",8508]
["10.49","Medium",8509]
["10.5","Low",8465]
["10.50","High",8510]
["10.51","Low",8511]
["10.52","Medium",8512]
["10.53","Medium",8513]
["10.54","High",8514]
["10.55","Low",8515]
["10.6","Very High",8466]
["10.7","Medium",8467]
["10.8","Medium",8468]
["10.9","Medium",8469]
["10.99","High",8516]
["11.1","High",8420]
["11.10","Medium",8429]
["11.11","Very High",8430]
["11.12","Low",8431]
["11.13","Low",8432]
["11.14","Medium",8433]
["11.15","Low",8434]
["11.16","Low",8435]
["11.17","Low",8436]
["11.2","Medium",8421]
["11.3","Medium",8422]
["11.4","Very High",8423]
["11.5","Medium",8424]
["11.6","Medium",8425]
["11.7","High",8426]
["11.8","Low",8427]
["11.9","Low",8428]
["11.99","High",8437]
["12.1","High",8438]
["12.10","High",8448]
["12.11","High",8449]
["12.12","High",8450]
["12.13","High",8451]
["12.14","High",8452]
["12.15","High",8453]
["12.16","High",8454]
["12.17","High",8455]
["12.18","High",8456]
["12.19","High",8457]
["12.2","High",8439]
["12.20","High",8458]
["12.21","High",8459]
["12.3","High",8441]
["12.4","High",8442]
["12.5","High",8443]
["12.6","High",8444]
["12.7","High",8445]
["12.8","High",8446]
["12.9","High",8447]
["12.99","High",8460]
["2.1","Very High",8296]
["2.1.9","Very High",11259]
["2.10","Medium",8304]
["2.11","Medium",8305]
["2.12","Low",8306]
["2.13","Low",8307]
["2.14","Low",8308]
["2.15","Low",8309]
["2.16","Medium",8310]
["2.2","Medium",8297]
["2.3","High",8295]
["2.4","Medium",8298]
["2.5","Medium",8299]
["2.6","Low",8300]
["2.7","High",8301]
["2.8","High",8302]
["2.9","Medium",8303]
["2.99","High",8311]
["3.1","High",8312]
["3.2","Very High",8313]
["3.3","High",8314]
["3.4","Low",8294]
["3.5","Medium",8315]
["3.6","High",8316]
["3.7","Very High",8317]
["3.8","Very High",8318]
["3.99","High",8319]
["4.1","High",8320]
["4.10","High",8329]
["4.11","Medium",8330]
["4.12","Very High",8331]
["4.13","Very High",8332]
["4.14","Very High",8333]
["4.15","Very High",8334]
["4.16","Very High",8335]
["4.17","Very High",8336]
["4.18","Very High",8337]
["4.19","Low",8338]
["4.2","Medium",8321]
["4.20","Very High",8339]
["4.21","High",8340]
["4.22","Low",8341]
["4.23","High",8342]
["4.24","High",8343]
["4.25","Low",8344]
["4.26","Low",8345]
["4.27","High",8346]
["4.3","Medium",8322]
["4.4","High",8323]
["4.5","Very High",8324]
["4.6","Medium",8325]
["4.7","High",8326]
["4.8","Medium",8327]
["4.9","Medium",8328]
["4.99","High",8347]
["5.1","Very High",8517]
["5.10","High",8526]
["5.11","Low",8527]
["5.12","Medium",8528]
["5.13","High",8529]
["5.14","Very High",8530]
["5.15","Medium",8531]
["5.16","Very High",8532]
["5.17","Very High",8533]
["5.18","High",8534]
["5.19","Medium",8535]
["5.2","Very High",8518]
["5.20","Medium",8536]
["5.21","Medium",8537]
["5.22","High",8539]
["5.23","Very High",8540]
["5.24","Very High",8541]
["5.25","Medium",8542]
["5.26","Medium",8543]
["5.27","Medium",8544]
["5.28","Very High",8545]
["5.29","High",8546]
["5.3","Low",8519]
["5.30","High",8547]
["5.31","High",8548]
["5.32","High",8549]
["5.33","High",8550]
["5.34","Low",8551]
["5.35","Medium",8552]
["5.36","Low",8553]
["5.37","Low",8554]
["5.38","High",8555]
["5.39","Very High",8556]
["5.4","High",8520]
["5.40","Very High",8557]
["5.41","Very High",8558]
["5.42","Medium",8559]
["5.43","High",8560]
["5.44","High",8561]
["5.45","Medium",8564]
["5.46","Medium",8565]
["5.47","Medium",8566]
["5.48","Medium",8567]
["5.5","Low",8521]
["5.6","Low",8522]
["5.7","Medium",8523]
["5.8","Medium",8524]
["5.9","Very High",8525]
["5.99","High",8568]
["6.1","Medium",8348]
["6.10","Low",8357]
["6.11","High",8358]
["6.12","Medium",8359]
["6.13","Low",8360]
["6.14","High",8361]
["6.15","High",8362]
["6.16","Very High",8363]
["6.17","Very High",8364]
["6.18","Medium",8365]
["6.19","Low",8366]
["6.2","High",8349]
["6.20","Medium",8367]
["6.21","High",8368]
["6.22","Medium",8369]
["6.3","Low",8350]
["6.4","High",8351]
["6.5","Medium",8352]
["6.6","Medium",8353]
["6.7","High",8354]
["6.8","High",8355]
["6.9","Low",8356]
["6.99","High",8370]
["7.1","High",8371]
["7.10","High",8380]
["7.11","High",8381]
["7.12","High",8382]
["7.13","Medium",8383]
["7.14","Medium",8384]
["7.15","High",8385]
["7.16","High",8386]
["7.17","High",8387]
["7.2","High",8372]
["7.3","Low",8373]
["7.4","Low",8374]
["7.5","Low",8375]
["7.6","Medium",8376]
["7.7","Low",8377]
["7.8","High",8378]
["7.9","High",8379]
["7.99","High",8388]
["8.1","Very High",8569]
["8.10","Very High",8578]
["8.100","Low",11227]
["8.101","Medium",11228]
["8.102","Low",11229]
["8.103","Low",11230]
["8.104","Low",11231]
["8.105","Medium",11232]
["8.106","Medium",11233]
["8.107","Low",11234]
["8.108","High",11235]
["8.109","Very High",11236]
["8.11","Medium",8579]
["8.110","High",11237]
["8.111","Medium",11238]
["8.112","High",11239]
["8.113","Medium",11240]
["8.114","Low",11241]
["8.115","High",11242]
["8.116","Medium",11243]
["8.117","Medium",11244]
["8.118","Medium",11245]
["8.119","High",11246]
["8.12","Medium",8580]
["8.120","High",11247]
["8.121","Medium",11248]
["8.122","High",11249]
["8.123","High",11250]
["8.124","Low",11251]
["8.125","High",11252]
["8.126","Medium",11253]
["8.127","Medium",11254]
["8.13","Medium",8581]
["8.14","Very High",8582]
["8.15","High",8583]
["8.16","Very High",8584]
["8.17","Low",8585]
["8.18","High",8586]
["8.19","High",8587]
["8.199","High",11255]
["8.2","Medium",8570]
["8.20","Medium",8588]
["8.21","High",8589]
["8.22","Very High",8590]
["8.23","Medium",8591]
["8.24","Medium",8592]
["8.25","Very High",8593]
["8.26","High",8594]
["8.27","Medium",8595]
["8.28","Medium",8596]
["8.29","High",8598]
["8.3","Very High",8571]
["8.30","High",8599]
["8.31","High",8600]
["8.32","Low",8601]
["8.33","Medium",8602]
["8.34","High",8603]
["8.35","Medium",8604]
["8.36","Medium",8605]
["8.37","High",8607]
["8.38","Medium",8608]
["8.39","Medium",8609]
["8.4","Medium",8572]
["8.40","High",8610]
["8.41","Medium",8611]
["8.42","Medium",8612]
["8.43","Very High",8613]
["8.44","High",8615]
["8.45","High",8616]
["8.46","Very High",8617]
["8.47","Very High",8618]
["8.48","Medium",8619]
["8.49","High",8620]
["8.5","Very High",8573]
["8.50","Medium",8621]
["8.51","Low",8622]
["8.52","Low",8623]
["8.53","Low",8624]
["8.54","High",8625]
["8.55","Low",11182]
["8.56","Medium",11183]
["8.57","Medium",11184]
["8.58","High",11185]
["8.59","High",11186]
["8.6","Medium",8574]
["8.60","High",11187]
["8.61","Medium",11188]
["8.62","Very High",11189]
["8.63","High",11190]
["8.64","Medium",11191]
["8.65","Low",11192]
["8.66","High",11193]
["8.67","High",11194]
["8.68","High",11195]
["8.69","Medium",11196]
["8.7","High",8575]
["8.70","Medium",11197]
["8.71","Very High",11198]
["8.72","Medium",11199]
["8.73","Medium",11200]
["8.74","High",11201]
["8.75","Medium",11202]
["8.76","Medium",11203]
["8.77","Medium",11204]
["8.78","Medium",11205]
["8.79","Medium",11206]
["8.8","Medium",8576]
["8.80","Medium",11207]
["8.81","Low",11208]
["8.82","Medium",11209]
["8.83","Low",11210]
["8.84","Low",11211]
["8.85","Medium",11212]
["8.86","Medium",11213]
["8.87","Medium",11214]
["8.88","Low",11215]
["8.89","High",11216]
["8.9","High",8577]
["8.90","High",11217]
["8.91","High",11218]
["8.92","Medium",11219]
["8.93","Low",11220]
["8.94","Low",11221]
["8.95","Medium",11222]
["8.96","Medium",11223]
["8.97","Low",11224]
["8.98","High",11225]
["8.99","Medium",11226]
["9.1","Low",8390]
["9.10","Medium",8399]
["9.11","Medium",8400]
["9.12","Medium",8401]
["9.13","Low",8402]
["9.14","Medium",8403]
["9.15","Medium",8404]
["9.16","High",8405]
["9.17","High",8406]
["9.18","Low",8407]
["9.19","Low",8408]
["9.2","Very High",8391]
["9.20","Medium",8409]
["9.21","Medium",8410]
["9.22","Low",8411]
["9.23","Low",8412]
["9.24","Medium",8413]
["9.25","Low",8414]
["9.26","Low",8415]
["9.27","Low",8416]
["9.28","Medium",8417]
["9.29","Low",8418]
["9.3","Very High",8392]
["9.4","High",8393]
["9.5","High",8394]
["9.6","Low",8395]
["9.7","Medium",8396]
["9.8","Medium",8397]
["9.9","Medium",8398]
["9.99","High",8419]

{"sheet":"Equipment_list","index":7,"n_rows":28,"n_cols":3,"rows_kept":28,"cut":false,"hidden":true,"merged":[]}
["TITLE","Equipment_list_description","ID"]
["Accommodation",null,12]
["Cargo Mach.",null,13]
["Critical Equip.",null,16]
["Deck - Machinery",null,18]
["Deck - Mooring Machinery",null,15]
["Deck - Pipe / Fittings",null,20]
["Documentation",null,21]
["E/R - Air Comp.",null,8]
["E/R - Aux. Engine",null,4]
["E/R - Aux. Mach.",null,7]
["E/R - Boiler",null,5]
["E/R - Main Engine",null,3]
["E/R - Pipes/ valves & fittings",null,9]
["E/R - Pumps",null,32]
["E/R - Purifier",null,6]
["Elect. Mach. & Equip.",null,10]
["Hull & Tanks",null,19]
["Inert Gas",null,14]
["LSA / FFA",null,17]
["Miscellaneous",null,22]
["Navigation - DGPS / EPFS / AIS",null,28]
["Navigation - ECDIS",null,25]
["Navigation - Echo Sounder / Speed Log",null,26]
["Navigation - GMDSS & Communication",null,23]
["Navigation - Others",null,11]
["Navigation - RADAR",null,24]
["Navigation - VDR / BNWAS",null,30]

{"sheet":"PSC_MOU","index":8,"n_rows":11,"n_cols":3,"rows_kept":11,"cut":false,"hidden":true,"merged":[]}
["TITLE","PSC_MOU_description","ID"]
["Asia and the Pacific",null,2]
["Caribbean",null,4]
["Europe and the North Atlantic",null,1]
["Latin America",null,3]
["The Black Sea region",null,6]
["The Indian Ocean",null,8]
["The Mediterranean",null,7]
["The Riyadh MoU",null,9]
["USCG",null,10]
["West and Central Africa",null,5]

{"sheet":"Inspection_type","index":9,"n_rows":13,"n_cols":2,"rows_kept":13,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Bunkering Audit",14]
["Cargo Audit",17]
["Engineering Audit",16]
["ISM Audit",2]
["ISPS Audit",3]
["IT Audit",10]
["MLC Audit",1]
["Mooring Audit",9]
["Nav Audit / Verification",8]
["Onboard Training",18]
["Ship Staff Insp.",15]
["Suptd. Insp.",13]

{"sheet":"Deficiency_Cause","index":10,"n_rows":8,"n_cols":3,"rows_kept":8,"cut":false,"hidden":true,"merged":[]}
["TITLE","Deficiency_Cause_description","ID"]
["Behaviour Based",null,1]
["Equipment Related",null,4]
["External Factors",null,5]
["Human Error",null,7]
["Inappropriate Procedure",null,8]
["Industry Issue",null,6]
["Knowledge Based",null,3]

{"sheet":"Observer_code","index":11,"n_rows":3,"n_cols":3,"rows_kept":3,"cut":false,"hidden":true,"merged":[]}
["TITLE","Observer_code_description","ID"]
["Owner / Marine / Tech. Suptd.",null,3]
["Ship Staff",null,2]

{"sheet":"Status_code","index":12,"n_rows":6,"n_cols":3,"rows_kept":6,"cut":false,"hidden":true,"merged":[]}
["TITLE","Status_code_description","ID"]
["Completed",null,6]
["Deferred to D D",null,5]
["In progress",null,3]
["Not Started",null,2]
["Waiting spare",null,4]

{"sheet":"PSC_ref_no","index":13,"n_rows":19,"n_cols":2,"rows_kept":19,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Alarms",9]
["Cargo operations including equipment",7]
["Certificates & Documentation",2]
["Dangerous Goods",13]
["Emergency Systems",5]
["Fire safety",8]
["ISM",16]
["ISPS",17]
["Life saving appliances",12]
["MLC, 2006",18]
["Other",19]
["Pollution Prevention",15]
["Propulsion and auxiliary machinery",14]
["Radio communication",6]
["Safety of Navigation",11]
["Structural condition",3]
["Water/Weathertight condition",4]
["Working and Living Conditions",10]

{"sheet":"Risk_value_of_obs","index":14,"n_rows":1,"n_cols":2,"rows_kept":1,"cut":false,"hidden":true,"merged":[]}
["Risk Value of observation","ID"]

{"sheet":"Year","index":15,"n_rows":18,"n_cols":1,"rows_kept":18,"cut":false,"hidden":true,"merged":[]}
["Year"]
[2014]
[2015]
[2016]
[2017]
[2018]
[2019]
[2020]
[2021]
[2022]
[2023]
[2024]
[2025]
[2026]
[2027]
[2028]
[2029]
[2030]

{"sheet":"Month","index":16,"n_rows":13,"n_cols":1,"rows_kept":13,"cut":false,"hidden":true,"merged":[]}
["Month"]
["Jan"]
["Feb"]
["Mar"]
["Apr"]
["May"]
["Jun"]
["Jul"]
["Aug"]
["Sep"]
["Oct"]
["Nov"]
["Dec"]

{"sheet":"Date_","index":17,"n_rows":32,"n_cols":1,"rows_kept":32,"cut":false,"hidden":true,"merged":[]}
["Date"]
["01"]
["02"]
["03"]
["04"]
["05"]
["06"]
["07"]
["08"]
["09"]
[10]
[11]
[12]
[13]
[14]
[15]
[16]
[17]
[18]
[19]
[20]
[21]
[22]
[23]
[24]
[25]
[26]
[27]
[28]
[29]
[30]
[31]

{"sheet":"Sheet1","index":18,"n_rows":24,"n_cols":6,"rows_kept":24,"cut":false,"hidden":true,"merged":[]}
[]
[null,"ID","E",null,"Date Recorded",1]
[null,"UNIQUE ID","F",null,"Type of Deficiency",2]
[1,"Date Recorded","G",null,"Observer code",3]
["ignore","Vessel Type","H",null,"Type of Inspection",4]
[null,"Internal / External","I",null,"Description of Deficiency",5]
[null,"Drydock","J",null,"Equipment Categories",6]
[null,"Information Sharing","K",null,"Area of Observation",7]
[null,"Critical_item","L",null,"Deficiency Cause",8]
[null,"Deficiency Type","M",null,"VIQ Ref Number",9]
[null,"Deficiency Cause","N",null,"Risk Value of Obs",10]
[null,"Inspection Type","O",null,"PSC Ref Number",11]
[null,"Equipments","P",null,"PSC MOU ID",12]
[null,"VIQ Reference Number","Q",null,"Action Taken or Required",13]
[null,"Risk Value of the observation","R",null,"Target Date",14]
[null,"PSC Reference Number","S",null,"PO Ref No.",15]
[null,"PSC MOU","T",null,"Status Code",16]
[null,"Observer Code","U",null,"Date Completed",17]
[null,"Target Date","V",null,"Drydock",18]
[null,"Status Code","W",null,"Info Sharing",19]
[null,"Description of Deficiency","X",null,"Critical Item Flag",20]
[null,"Action taken / required","Y",null,"Audit Type",21]
[null,"PO ref no","Z"]
[null,"Date completed","AA"]

{"sheet":"Ship_information","index":19,"n_rows":2,"n_cols":3,"rows_kept":2,"cut":false,"hidden":true,"merged":[]}
["Ship_ID","Ship_Name","FILE_NAME"]
["98","AZIMUTH (01-07-2020)","98_1593577106723.xlsm"]

{"sheet":"External_Deficiency_type","index":20,"n_rows":5,"n_cols":3,"rows_kept":5,"cut":false,"hidden":true,"merged":[]}
["TITLE","Type of deficiency_description","ID"]
["Condn of Class / Memo",null,5]
["Defect",null,1]
["Non Conformity",null,2]
["Observation",null,3]

{"sheet":"External_Inspection_type","index":21,"n_rows":11,"n_cols":2,"rows_kept":11,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Cargo Audit",17]
["Flag State Insp.",5]
["ISM Audit",2]
["ISPS Audit",3]
["MLC Audit",1]
["Nav Audit / Verification",8]
["OM Insp. (Eg. SIRE / CDI etc.)",6]
["Others (Eg. Insurance etc.)",12]
["PSC Inspection",4]
["Terminal Insp.",11]

{"sheet":"External_Observer_code","index":22,"n_rows":7,"n_cols":3,"rows_kept":7,"cut":false,"hidden":true,"merged":[]}
["TITLE","Observer_code_description","ID"]
["Class Surveyor",null,4]
["FSC Inspector",null,5]
["Others (Eg. Insurance etc.)",null,9]
["PSC Insp.",null,6]
["SIRE / CDI Insp.",null,8]
["Terminal Insp.",null,7]

{"sheet":"Sheet Version","index":23,"n_rows":2,"n_cols":2,"rows_kept":2,"cut":false,"hidden":true,"merged":[]}
["Version","Title"]
["2.0","Version 2.0"]