{"text_format":"1","workbook":"xlsx","n_sheets":24,"sheets":["Mainsheet","Completed","Calc","Areaofobs","Vessel_type","Deficiency_type","VIQrefno","Equipment_list","PSC_MOU","Inspection_type","Deficiency_Cause","Observer_code","Status_code","PSC_ref_no","Risk_value_of_obs","Year","Month","Date_","Sheet1","Ship_information","External_Deficiency_type","External_Inspection_type","External_Observer_code","Sheet Version"],"not_rendered":{"charts":0,"images":6,"macros":1,"external_links":0,"defined_names":12,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Mainsheet","index":0,"n_rows":34,"n_cols":28,"rows_kept":34,"cut":false,"hidden":false,"merged":[[10,8,10,9],[10,12,10,13],[12,6,12,27],[8,6,8,27]]}
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,"Defect - Damage Monitoring Sheet"]
[]
[null,null,null,null,null,null,null,"Date of Report","2020-12-17",null,null,"Ship Name","DHT TAIGA (17-12-2020)"]
[]
[null,null,null,null,null,null,"VERSION : 2.0"]
[]
[]
[]
[null,null,null,null,"ID","UNIQUE ID","Date Recorded","Type of Deficiency","Observer code","Type of Inspection","Description of Deficiency","Equipment Categories","Area of Observation","Deficiency Cause","VIQ Ref Number","Risk Value of Obs","PSC Ref Number","PSC MOU ID","Action Taken or Required","Target Date","PO Ref No.","Status Code","Date Completed","Drydock","Info Sharing","Critical Item","Audit Type","Superintendent Remarks"]
[null,null,null,null,9928,"48_20/1/2020 6:07:05 PM","2020-04-19","Guarantee Claim","Ship Staff","Ship Staff Insp.","APK Tank Level Sensor (AP-LVL-01) Faulty","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related",8.1199999999999992,"Medium","Not Applicable","Not Applicable","Isolation converter received and installed in the circuit , Aft peak level found working ok in both Tank Radar and BWTS without any issue , however it is interfering with aft draft gauge and aft gauge giving erratic readings .","2021-01-30","STAI200077","Waiting spare",null,"No","No","No","Internal","Awaiting maker advise. Target date revised"]
[null,null,null,null,13185,"48_17/07/2020 9:56:16 AM","2020-07-10","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Cargo line dresser coupling bolts are rusted at various locations, to be renewed.","Deck - Pipe / Fittings","General Appearance","Equipment Related",null,null,"Not Applicable","Not Applicable","Job in progress, Derusting & painting of U clamp & fittings completed IWO 4 & 5 Across COT.","2021-01-30",null,"In progress",null,"No","No","No","Internal"]
[null,null,null,null,14004,"48_15/09/2020 11:55:04 AM","2020-09-05","Defect","Ship Staff","Ship Staff Insp.","Hydro blaster (Combo for high pressure waterjet) not generating sufficient pressure for blasting operation.","Deck - Machinery","General Appearance","Equipment Related",null,null,"Not Applicable","Not Applicable","Consulted the maker. They have sent the spares list to be ordered. same will be ordered after 1st Jan 2021.","2021-05-04",null,"Waiting spare",null,"No","No","No","Internal","Any spares required?"]
[null,null,null,null,14008,"48_15/9/2020 2:51:24 PM","2020-09-09","Defect","Ship Staff","Ship Staff Insp.","ME FO viscosity control unit malfunctioning.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related",null,null,"Not Applicable","Not Applicable","Changed the viscotherm along with new potentiometer. Still not working. Found ES11 ( electronic positioner ) not working. Spare ordered","2021-05-09","STAI200274","Waiting spare",null,"No","No","No","Internal"]
[null,null,null,null,14161,"48_23/9/2020 5:05:04 PM","2020-09-17","Defect","Ship Staff","Ship Staff Insp.","ME AUX BLOWER NO 1 RUNNING INDICATION  IN AMS (ACONIS) IS NOT SHOWING FOUND THAT RELAY CONTACTOR DEFECTIVE.HIMX40 ","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related",null,null,"Not Applicable","Not Applicable","Requaird to replaced with new Relay contactor RO Raised for requaried spares.","2021-05-17","STAI200218","Waiting spare",null,"No","No","No","Internal"]
[null,null,null,null,14164,"48_27/9/2020 2:38:43 PM","2020-09-27","Defect","Ship Staff","Ship Staff Insp.","Grey water pump not pumping eventhough it was checked and overhauled how many time and still no success to make it operational. ","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related",null,null,"Not Applicable","Not Applicable","New type of pump to be install","2021-06-27",null,"Not Started",null,"No","No","No","Internal"]
[null,null,null,null,14165,"48_3/10/2020 2:18:03 PM","2020-09-27","Defect","Ship Staff","Ship Staff Insp.","All top bracing found leaking","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related",null,null,"Not Applicable","Not Applicable","Top bracing to be overhaul and parts to renew. Unit 2 & 3 overhauled. NO.1 and 4 has to be overhaul when spare receive.","2021-05-27","STAI200224","Waiting spare",null,"No","No","No","Internal"]
[null,null,null,null,14168,"48_28/9/2020 1:48:42 PM","2020-09-27","Defect","Ship Staff","Ship Staff Insp.","Soot Blower #6( For HP) for EGB not operational . It is getting stuck while in use ","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related",null,null,"Not Applicable","Not Applicable","Need to remove the soot blower from place, ease it  and make it operational","2021-06-30",null,"In progress",null,"No","No","No","Internal"]
[null,null,null,null,14167,"48_4/10/2020 2:55:11 PM","2020-09-30","Defect","Ship Staff","Ship Staff Insp.","Thermostat for JCW preheater for Aux DG is not working.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related",null,null,"Not Applicable","Not Applicable","need replacement. Spares ordered.","2021-05-01","STAI200225","Waiting spare",null,"No","No","No","Internal"]
[null,null,null,null,14169,"48_4/10/2020 2:58:28 PM","2020-09-30","Defect","Ship Staff","Ship Staff Insp.","Unable to do EGB soot blow from ECR. \t","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related",null,null,"Not Applicable","Not Applicable","Reset the system from local panel and ECR panel. HMi restarted. Still not operational from ECR. Email sent for further advise. Troubleshooting in progress with makers advise. waiting for suitable anchorage.","2021-05-05",null,"In progress",null,"No","No","No","Internal"]
[null,null,null,null,null,"48_06/11/2020 16:21:29","2020-11-03","Defect","Ship Staff","Ship Staff Insp.","EGB soot blower lances are wasted and detached. ","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related",null,null,"Not Applicable","Not Applicable","SOOT BLOWER LANCES TO BE RENEWED. OFFICE INFORMED,  . NEW LANCES TO BE ORDERED","2021-05-03",null,"Not Started",null,"No",null,null,"Internal"]
[null,null,null,null,null,"48_27/11/2020 16:59:47","2020-11-28","Defect","Ship Staff","Ship Staff Insp.","GALLEY BEAKING OVEN NO 2 NOT OPRATIONAL ","Accommodation","General Appearance","Equipment Related",null,null,"Not Applicable","Not Applicable","Requried to replaced  heatting coils PO raised for new spare coils","2021-05-31","STAI200273","Waiting spare",null,"No",null,null,"Internal"]
[null,null,null,null,null,"48_18/12/2020 01:36:44","2020-12-02","Defect","Ship Staff","Ship Staff Insp.","Spider coupling for Aft and FWD hydraulic pumps damaged. Same needs to be replaced","Deck - Machinery","Eng. / Strg. Comp.","Equipment Related",null,null,"Not Applicable","Not Applicable","Informed office. Need to procure the spider couplings","2021-03-01",null,"Waiting spare",null,"No",null,null,"Internal"]
[null,null,null,null,null,"48_03/12/2020 3:14:45 PM","2020-12-03","Breakdown","Ship Staff","Ship Staff Insp.","A-Deck Crew laundry washing machine not operational. PCB & Motor found damaged due to water ingress","Accommodation","MLC Related","Equipment Related",null,null,"Not Applicable","Not Applicable","New Machine to be ordered. Will be ordered after 1st Jan 2021.","2021-05-02",null,"Not Started",null,"No",null,null,"Internal"]
[null,null,null,null,null,"48_15/12/2020 17:59:19","2020-12-16","Defect","Ship Staff","Ship Staff Insp.","M/E VISCOSITY NOT SHOWING (SHOWING ZERO) ON CONTROLLER","Miscellaneous","Eng. / Strg. Comp.","Equipment Related",null,null,"Not Applicable","Not Applicable","VISCOSENSOR MALFUCNTIONS NEED TO REPLACE. SPARES WILL BE ORDERED AFTER 1ST JAN 2021.","2021-03-31",null,"Waiting spare",null,"No",null,null,"Internal"]
[null,null,null,null,null,"48_15/12/2020 18:10:24","2020-12-16","Defect","Ship Staff","Ship Staff Insp.","NO 2S COT ullage error in SAAB system. No responce from 2S TGU  unit. ","Cargo Mach.","Cargo / Ballast Systems","Equipment Related",8.1199999999999992,"Medium","Not Applicable","Not Applicable","Swap test carried out by swapping 2P TGE unit to 2S TGU. 2S TGE unit is faulty & not giving signal to SCC unit. New TGE unit required. Awaiting office advice for supply of new TGE unit","2021-03-31",null,"In progress",null,"No",null,null,"Internal"]
[null,null,null,null,null,"48_18/12/2020 11:09:05 PM","2020-12-16","Defect","Ship Staff","Ship Staff Insp.","During grit blasting of Hydraulic lines on deck. 3 holes observed in  Hydraulic oil return line for aft mooring winches (Spring lines) ","Deck - Pipe / Fittings","Mooring","Equipment Related",11.4,"Very High","Not Applicable","Not Applicable","Section of pipe removed & repair work in progress in E/R workshop. New pipe to be inserted in the defected section of pipe.","2020-12-20",null,"In progress",null,"No",null,null,"Internal"]

{"sheet":"Completed","index":1,"n_rows":255,"n_cols":28,"rows_kept":255,"cut":false,"hidden":false,"merged":[[10,8,10,9],[10,12,10,13],[12,6,12,27],[8,6,8,27]]}
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,"Defect - Damage Monitoring Sheet"]
[]
[null,null,null,null,null,null,null,"Date of Report","07-Oct-2020",null,null,"Ship Name","DHT TAIGA (19-09-2020)"]
[]
[null,null,null,null,null,null,"VERSION : 2.0"]
[]
[]
[]
[null,null,null,null,"ID","UNIQUE ID","Date Recorded","Type of Deficiency","Observer code","Type of Inspection","Description of Deficiency","Equipment Categories","Area of Observation","Deficiency Cause","VIQ Ref Number","Risk Value of Obs","PSC Ref Number","PSC MOU ID","Action Taken or Required","Target Date","PO Ref No.","Status Code","Date Completed","Drydock","Info Sharing","Critical Item","Audit Type","Superintendent Remarks"]
[null,null,null,null,6226,"48_24/10/2019 9:47:45 PM","2019-01-04","Defect","Ship Staff","Ship Staff Insp.","Anemometer- Wind speed transmitter found not working","Navigation - Others","Navigation","Equipment Related","4.7","High","","","Old repaired Anemometer transmitter installed. Tested and found operational.","2019-01-14","","Completed","2019-01-13","No","No","No","Internal"]
[null,null,null,null,6227,"48_24/10/2019 9:52:15 PM","2019-01-11","Defect","Ship Staff","Ship Staff Insp.","FWD air horn non operational","Navigation - Others","Navigation","Equipment Related","10.37","Medium","","","Air horn compressor and motor overhauled , fitted back and tried out, working satisfactory.","2019-01-18","","Completed","2019-01-18","No","No","No","Internal"]
[null,null,null,null,6228,"48_24/10/2019 9:57:34 PM","2019-01-12","Defect","Ship Staff","Ship Staff Insp.","IG Fan drain line in 3rd deck platform found leaking due to crack in the pipeline.","Inert Gas","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","New pipe fabricated wid stainless steel pipe and flange . Pipe replaced with fabricated one and tested, found satisfactory.","2019-01-12","","Completed","2019-01-12","No","No","No","Internal"]
[null,null,null,null,6229,"48_24/10/2019 9:59:53 PM","2019-01-12","Defect","Ship Staff","Ship Staff Insp.","Main engine unit no.4 cyl.jacket inlet pipe leaking from flange joint.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Gasket replaced and boxed back with stainless steel bolts.","2019-01-16","","Completed","2019-01-16","No","No","No","Internal"]
[null,null,null,null,6230,"48_24/10/2019 10:02:27 PM","2019-01-14","Defect","Ship Staff","Ship Staff Insp.","Hydraulic oil leakage from FWD windlass (PORT) High/Low control lever (DIRECTIONAL CONTROL VALVE)","Deck - Machinery","Mooring","Equipment Related","9.2","Very High","","","Both seals and o rings changed for the Directional control valve andf tested, and found working satisfactory.","2019-01-18","","Completed","2019-01-18","No","No","No","Internal"]
[null,null,null,null,6160,"48_24/10/2019 10:38:50 PM","2019-01-28","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Main deck port side,U - Clamps on hydraulic lines, FW lines and air lines found rusted.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related,External Factors","11.5","Medium","","","All rusts removed and painted.","2019-04-28","","Completed","2019-02-26","No","No","No","Internal"]
[null,null,null,null,6161,"48_24/10/2019 10:41:44 PM","2019-01-28","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","SIP'S around the accommodation not clearly marked.","Hull & Tanks","General Appearance","External Factors,Human Error","11.6","Medium","","","SIP markings completed.","2019-04-28","","Completed","2019-03-01","No","No","No","Internal"]
[null,null,null,null,6162,"48_24/10/2019 10:43:36 PM","2019-01-28","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ME UNIT # 6 Starting air valve solenoid cable was reported damaged, junction box found open and new cable laid externally, cable to be routed properly.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Cable renewed.","2019-04-28","","Completed","2019-03-11","No","No","No","Internal"]
[null,null,null,null,6163,"48_24/10/2019 10:46:03 PM","2019-01-28","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Mooring wires dry and rusty not greased using wire rope greaser.","Deck - Machinery,Deck - Mooring Machinery","Mooring","Equipment Related,Human Error","9.17","High","","","All mooring wires greasing carried out.","2019-04-28","","Completed","2019-03-22","No","No","No","Internal"]
[null,null,null,null,6164,"48_24/10/2019 10:48:36 PM","2019-01-28","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Port MGPS CU-AL anode showing error.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.37","Medium","","","Defective control PCB for CU and AL-Anode replaced with new spare Port MGPS is operational.","2019-04-28","","Completed","2019-04-22","No","No","No","Internal"]
[null,null,null,null,6165,"48_24/10/2019 10:50:32 PM","2019-01-28","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Dead man alarm indication light in pump room entrance not operational.","Elect. Mach. & Equip.","Cargo / Ballast Systems","Equipment Related","11.11","Very High","","","Received spare. Modified the switch and fitted back. It is working now.","2019-10-31","","Completed","2019-09-09","No","No","No","Internal"]
[null,null,null,null,6231,"48_24/10/2019 10:06:01 PM","2019-01-28","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","COPT # 2 Discharge line flange valve no.260 in pump room found traces of oil leakage.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.44","High","","","Oil traces cleaned and flange tightened,no oil leakage","2019-04-28","","Completed","2019-01-31","No","No","No","Internal"]
[null,null,null,null,6232,"48_24/10/2019 10:11:45 PM","2019-01-28","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Stenciling of various remote sounding boxes for ballast tanks missing","Hull & Tanks","General Appearance","Human Error","11.7","High","","","Steciling carried out for all remote sounding boxes for ballast tanks","2019-04-28","","Completed","2019-01-29","No","No","No","Internal"]
[null,null,null,null,6233,"48_24/10/2019 10:14:28 PM","2019-01-28","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","One light in pump room 2nd deck not working.","Elect. Mach. & Equip.","Cargo / Ballast Systems","Equipment Related","11.11","Very High","","","Light renewed","2019-01-28","","Completed","2019-01-29","No","No","No","Internal"]
[null,null,null,null,6234,"48_24/10/2019 10:17:16 PM","2019-01-28","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Pressure regulator in air line for sea chest testing not fitted","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related,Human Error","6.4","High","","","Pressure regulator fitted in air line for sea chest testing.","2019-04-28","","Completed","2019-02-12","No","No","No","Internal"]
[null,null,null,null,6235,"48_24/10/2019 10:19:29 PM","2019-01-28","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Windlass pinion bearing found not greased and grease point not clearly marked.","Deck - Machinery,Deck - Mooring Machinery","Mooring","Equipment Related,Human Error","9.2","Very High","","","Windlass pinion bearing greasing carried out and grease point marked.","2019-04-28","","Completed","2019-02-06","No","No","No","Internal"]
[null,null,null,null,6236,"48_24/10/2019 10:24:15 PM","2019-01-28","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Helicopter equipement CO2 extinguishers not as per requirement","LSA / FFA","Safety / LSA / FFA","Human Error,Knowledge Based","5.4","High","","","CO2 extinguishers installed as per requirement.","2019-04-28","","Completed","2019-02-11","No","No","No","Internal"]
[null,null,null,null,6237,"48_24/10/2019 10:26:52 PM","2019-01-28","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ME UNIT # 3 Starting air valve solenoid cable was reported damaged, junction box found open and new cable laid externally, cable to be routed properly.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related,Inappropriate Procedure","10.32","Very High","","","Cable renewed soon after receiving new cable.","2019-04-28","","Completed","2019-02-03","No","No","No","Internal"]
[null,null,null,null,6238,"48_24/10/2019 10:29:52 PM","2019-01-28","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","EGB bellow between LP and HP evaporator had traces of leakage, to be checked , cleaned and painted.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Bellow inspected, no leakes found.Bellow area cleaned and painted.","2019-04-28","","Completed","2019-02-17","No","No","No","Internal"]
[null,null,null,null,6166,"48_24/10/2019 10:59:49 PM","2019-01-30","Defect","Ship Staff","Ship Staff Insp.","Port Side ECDIS unit on Bridge Buzzer for alarm is not working.","Elect. Mach. & Equip.","Navigation","Equipment Related","","","","","Replaced operation circuit for ECDIS 2 (part No. OPU CCK-976 (PC640,7PCRD1796B)). Buzzer working satisfactorily.","2019-10-31","","Completed","2019-09-03","No","No","No","Internal"]
[null,null,null,null,6167,"48_24/10/2019 11:05:55 PM","2019-02-06","Defect","Ship Staff","Ship Staff Insp.","Main engine # 6 unit jacket water outlet temperature reading shows erratic","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Temperature sensor renewed and working satisfactory.","2019-02-06","","Completed","2019-02-06","No","No","No","Internal"]
[null,null,null,null,6168,"48_24/10/2019 11:07:47 PM","2019-02-16","Defect","Ship Staff","Ship Staff Insp.","Vacuum toilet system port side line in operational","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Vacuum toilet line - Port side blockage rectified by flushing with water and air","2019-02-16","","Completed","2019-02-16","No","No","No","Internal"]
[null,null,null,null,6169,"48_24/10/2019 11:09:56 PM","2019-02-18","Defect","Ship Staff","Ship Staff Insp.","Sewage overboard valve - minor leakage ( 2/3 drop/day) through the storm valve body at the Engine room bottom floor on port side","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Temporary measures have been taken with UW and normal steel putty and currently no sign of leakage. New valve has been ordered. In order to renew the valve plugging of Overboard line is required.Sewage overboard valve renewed at Singapore anchorage.","2019-05-31","","Completed","2019-05-21","No","No","No","Internal"]
[null,null,null,null,6170,"48_24/10/2019 11:11:49 PM","2019-02-21","Defect","Ship Staff","Ship Staff Insp.","Main CSW pump no.1 - Discharge pressure gauge showing incorrect value","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Root valve for the pressure gauge renewed and line blown through - Gauge is operational.","2019-02-22","","Completed","2019-02-21","No","No","No","Internal"]
[null,null,null,null,6171,"48_24/10/2019 11:38:34 PM","2019-03-01","Defect","Ship Staff","Ship Staff Insp.","Fresh water generator 1- Ejector pump sea water suction valve not holding, unable to isolate the pump.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","valve Renewed","2019-10-15","","Completed","2019-10-31","No","No","No","Internal"]
[null,null,null,null,6172,"48_24/10/2019 11:42:28 PM","2019-03-02","Defect","Ship Staff","Ship Staff Insp.","Citadel Iridium Phone displaying \"SIM Card Blocked\" and can't be used.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","7.6","Medium","","","Troubleshooting carried out with the help of IT departments. Phone is operational now.","2019-03-20","","Completed","2019-03-31","No","No","No","Internal"]
[null,null,null,null,6173,"48_24/10/2019 11:47:00 PM","2019-03-07","Defect","Ship Staff","Ship Staff Insp.","ME Jacket pre heater steam inlet pressure gauge needle found broken.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Pressure gauge renewed.","2019-03-07","","Completed","2019-03-08","No","No","No","Internal"]
[null,null,null,null,6174,"48_24/10/2019 11:49:58 PM","2019-03-10","Defect","Ship Staff","Ship Staff Insp.","ME- Aft Aux. Blower cooling fan blades found damaged","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","ME- Aft Aux. Blower cooling fan renewed and tested.","2019-03-10","","Completed","2019-03-11","No","No","No","Internal"]
[null,null,null,null,6175,"48_25/10/2019 8:39:58 AM","2019-03-24","Defect","Ship Staff","Ship Staff Insp.","TG condenser –Condensate water inlet to vapour chamber pressure gauge found faulty","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Pressure gauge renewed.","2019-03-24","","Completed","2019-03-24","No","No","No","Internal"]
[null,null,null,null,6176,"48_25/10/2019 8:54:11 AM","2019-03-26","Defect","Ship Staff","Ship Staff Insp.","Main Engine -Fuel oil Viscotherm is showing erratic reading.","Elect. Mach. & Equip.,E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.37","Medium","","","Sensor received and changed. Showing viscosity correctly","2019-06-25","","Completed","2019-07-10","No","No","No","Internal"]
[null,null,null,null,6177,"48_25/10/2019 8:56:53 AM","2019-03-27","Defect","Ship Staff","Ship Staff Insp.","Auxiliary Engine - T/C Exhaust gas inlet temperature sensor -A found faulty","E/R - Aux. Engine,Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.37","Medium","","","Sensor renewed and is operational.","2019-03-28","","Completed","2019-03-27","No","No","No","Internal"]
[null,null,null,null,6178,"48_25/10/2019 8:59:47 AM","2019-03-29","Defect","Ship Staff","Ship Staff Insp.","WBT 3 (P) and WBT 5 (P) gauges showing erratic reading","Hull & Tanks","Cargo / Ballast Systems","Equipment Related","8.8","Medium","","","5P & 3P WBT sensor renewed.","2019-10-31","","Completed","2019-10-01","No","No","No","Internal"]
[null,null,null,null,6179,"48_25/10/2019 9:01:57 AM","2019-04-01","Defect","Ship Staff","Ship Staff Insp.","Port windlass brake cylinder top cover seal slightly leaking","Deck - Machinery,Deck - Mooring Machinery","Mooring","Equipment Related","9.2","Very High","","","Scraper ring, wear ring and rod seal renewed for top cover and tested - working satisfactory.","2019-04-02","","Completed","2019-04-01","No","No","No","Internal"]
[null,null,null,null,8610,"48_Thu Sep 12 2019 17:50:29 GMT+0000 (Coordinated Universal Time)","2019-04-11","Defect","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","No evidence when the workshop and upper deck oxylacy regulators were last inspected annually or renewed in the last 5 years.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Inappropriate Procedure","5.26","Medium","","","New regulators for Oxygen and Acetylene were\n\nordered and were received by the vessel on 19th April 2019 at Singapore and the regulators\n\nwere replaced the same day.\n\nAll the documentation regarding the renewal of these regulators has been filed on board for\n\nrecords. Additionally the job for annual inspection and five yearly renewal of these regulators\n\nhas been added in the PMS for proper record keeping.","2019-04-26","","Completed","2019-04-19","No","No","No","External"]
[null,null,null,null,6180,"48_25/10/2019 9:03:51 AM","2019-04-16","Defect","Ship Staff","Ship Staff Insp.","Pump Room Blower Motor Low Insulation.","Deck - Machinery,Elect. Mach. & Equip.","Cargo / Ballast Systems","Equipment Related","10.38","Medium","","","Pump Room fan motor inside the terminal box one wire connection to motor winding got grounded, same replaced with new wire and motor both bearing changed with new spare, blower is operational","2019-04-28","","Completed","2019-04-24","No","No","No","Internal"]
[null,null,null,null,6181,"48_25/10/2019 9:07:39 AM","2019-04-28","Defect","Ship Staff","Ship Staff Insp.","Forward whistle horn , reported not working","Elect. Mach. & Equip.","Navigation","Equipment Related","","","","","Motor electrical connection disconnected to facilitate the repair work of the whistle. Complete unit removed from its place and taken to workshop. Dismantled the unit and found connecting rod bearing completely damaged. Same replaced with old","2019-04-29","","Completed","2019-04-29","No","No","No","Internal"]
[null,null,null,null,8601,"48_Mon Dec 09 2019 23:18:36 GMT+0000 (Coordinated Universal Time)","2019-04-30","Defect","Ship Staff","Nav Audit / Verification","Course Recorder was not marked and entries made after every Navigation watch.","Documentation","Navigation","Human Error","4.7","High","","","Missed entry was entered by concerned officer. Officer briefed regarding same. All officers briefed regarding the importance of making appropriate entries in log books and other records prior handing over watch so as to prevent recurrence.","2019-05-15","","Completed","2019-05-03","No","No","No","Internal"]
[null,null,null,null,8602,"48_Thu Sep 12 2019 23:21:55 GMT+0000 (Coordinated Universal Time)","2019-04-30","Defect","Ship Staff","Nav Audit / Verification","1 ENC Permit in ECDIS not updated.","Navigation - ECDIS","Navigation","External Factors","4.12","Very High","","","Navtor informed regarding missing ENC update and assistance requested to recify same. All permits received and uploaded in ECDIS system. All ECDIS ENC permits  updated to latest corrections. All were briefed : All officers to be well conversant with ECDIS and Navtor so as to ensure when receiving and updating ECDIS, all ENC permits are updated till latest week. Any missing update to be immediately reported to Navtor for rectifing same.","2019-05-15","","Completed","2019-04-30","No","No","No","Internal"]
[null,null,null,null,8603,"48_Mon Dec 09 2019 23:26:04 GMT+0000 (Coordinated Universal Time)","2019-04-30","Defect","Ship Staff","Nav Audit / Verification","No.2 ECDIS (Backup) Audible alarm not working.","Navigation - ECDIS","Navigation","Equipment Related","4.7","High","","","All officers informed regarding inoperational audible alarm on No.2 ECDIS. No.1 ECDIS alarm checked and found working satisfactory. Office informed regarding same and assistance requested to rectify the faulty audible alarm. Attended by maker's technician and issue resolved.","2019-06-30","","Completed","2019-05-21","No","No","No","Internal"]
[null,null,null,null,6182,"48_25/10/2019 9:09:58 AM","2019-05-01","Defect","Ship Staff","Ship Staff Insp.","CONNING DISPLAY ,PROCESSOR FAN FAIL","E/R - Aux. Mach.,Navigation - Others","Eng. / Strg. Comp.","Equipment Related","11.1","High","","","processor fan replaced by CODAR technician at Singapore","2019-08-01","STAI190081","Completed","2019-05-21","No","No","No","Internal"]
[null,null,null,null,8596,"48_Mon Dec 09 2019 18:06:28 GMT+0000 (Coordinated Universal Time)","2019-05-05","Defect","PSC Insp.","PSC Inspection","A Steam return pipe connection in work shop leaking","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Human Error","11.4","Very High","Other","","Cargo discharge stopped and steam line de-pressurised and isolated. Leaking flange gasket renewed and leak rectified / tested. Vessel resumed heating of slop tanks and Discharge operations","2019-05-05","","Completed","2019-05-05","No","No","No","External"]
[null,null,null,null,8597,"48_Mon Dec 09 2019 18:09:46 GMT+0000 (Coordinated Universal Time)","2019-05-05","Defect","PSC Insp.","PSC Inspection","The operating direction mark for ventilator of steering gear room not visible.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Human Error","11.6","Medium","Water/Weathertight condition","","Operating direction mark for ventilator was repainted immediately and PSC inspector verified same. ","2019-05-06","","Completed","2019-05-05","No","No","No","External"]
[null,null,null,null,6183,"48_25/10/2019 8:16:31 AM","2019-05-10","Defect","Ship Staff","Ship Staff Insp.","Aux Boiler F.O. pump supply Mechanical seal leaking","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Mechanical Seal changed , P/P tried out satisfactory","2019-08-31","","Completed","2019-07-26","No","No","No","Internal"]
[null,null,null,null,6184,"48_25/10/2019 11:38:10 AM","2019-05-10","Defect","Ship Staff","Ship Staff Insp.","Frequency controllers for MSW pumps #3 not working","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.37","Medium","","","FREQUENCY CONTROLLER FOR NO1 AND 2 ATTENDED ON 15/06/2019 AND NOW WORKING SATISFACTORY, As per office instructions Frequency controller not to be changed. Pump to","2019-08-30","","Completed","2019-06-15","No","No","No","Internal"]
[null,null,null,null,6185,"48_25/10/2019 11:41:49 AM","2019-05-10","Defect","Ship Staff","Ship Staff Insp.","VACUUMARATOR PUMP NO.1 END PLATE BADLY WORN OUT .","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Pump working satisfactory. Parts kept as spare. To be changed if issue arises","2019-08-25","","Completed","2019-07-07","No","No","No","Internal"]
[null,null,null,null,6186,"48_25/10/2019 11:45:20 AM","2019-05-10","Defect","Ship Staff","Ship Staff Insp.","IGS ECR Main control valve leaking when IG is venting to atmosphere and main blower in use","Inert Gas","Cargo / Ballast Systems","Equipment Related","10.32","Very High","","","Valve seat renewed. Tried out . No leakage observed","2019-08-30","STAI 190078","Completed","2019-08-05","No","No","No","Internal"]
[null,null,null,null,6187,"48_25/10/2019 11:48:09 AM","2019-05-10","Defect","Ship Staff","Ship Staff Insp.","GE fuel line Pr regulating v/v 9k leaking","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Confirmed the operation during LSMGO and HFO. Found not leaking. Holdingnow. Under observation. Vessel received spare. Kept standby","2019-10-31","STAI190112","Completed","2019-08-20","No","No","No","Internal"]
[null,null,null,null,6224,"48_25/10/2019 12:03:13 AM","2019-05-10","Defect","Ship Staff","Ship Staff Insp.","Aux Boiler Feed water pumps motor #1 and #3 cooling Fan damaged","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Received the spare and changed the cooling fan. ","2019-11-30","","Completed","2019-11-07","No","No","No","Internal"]
[null,null,null,null,6188,"48_25/10/2019 11:51:49 AM","2019-05-12","Defect","Ship Staff","Ship Staff Insp.","Control air dryer #1 not working","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.37","Medium","","","Spares received and changed. Found working satisfactory.","2019-10-31","","Completed","2019-10-05","No","No","No","Internal"]
[null,null,null,null,6189,"48_25/10/2019 11:54:11 AM","2019-05-21","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","No 1 boiler burner platform has steam / leakage. Looks like same is from steam regulating valve.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Gasket to be renewed.","2019-05-31","","Completed","2019-05-24","No","No","No","Internal"]
[null,null,null,null,6190,"48_25/10/2019 11:56:47 AM","2019-05-21","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Air bottles auto drain valve is kept shut. Same to be opened and all the crew to be advised accordingly.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","VALVES OPENED AND CREW ADVISED OF THE OPERATION","2019-05-28","","Completed","2019-05-22","No","No","No","Internal"]
[null,null,null,null,6191,"48_25/10/2019 12:00:28 PM","2019-05-21","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Area below the blower in steering Gear room needs to be cleaned.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Area cleaned and painted","2019-07-21","","Completed","2019-06-03","No","No","No","Internal"]
[null,null,null,null,6192,"48_25/10/2019 1:36:51 PM","2019-05-21","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","In steam line there is steam / water leak from dump bypass valve and air ejector steam inlet valve. To be rectified by closing main steam stop valve","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","gasket renewed","2019-07-21","","Completed","2019-05-30","No","No","No","Internal"]
[null,null,null,null,6193,"48_25/10/2019 1:40:19 PM","2019-05-21","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Provision compressor low pressure gauge to renew","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Pressure Gauge renewed","2019-06-21","","Completed","2019-06-02","No","No","No","Internal"]
[null,null,null,null,6194,"48_25/10/2019 1:44:14 PM","2019-05-21","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Port side bunker manifold pressure gauge to renew, as same showing wrong indication.","Deck - Pipe / Fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Pressure Gauge renewed","2019-06-21","","Completed","2019-05-30","No","No","No","Internal"]
[null,null,null,null,6195,"48_25/10/2019 1:50:47 PM","2019-05-21","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","All 3 Aft winches gear case relief valve spring is missing. To replace.","Deck - Machinery","Mooring","Equipment Related","9.14","Medium","","","Springs replaced.","2019-06-21","","Completed","2019-06-14","No","No","No","Internal"]
[null,null,null,null,6196,"48_25/10/2019 1:56:01 PM","2019-05-21","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Stbd side pump room blower motor top cover is temporarily repaired by cold work. New cover to fabricate and fit.","Deck - Machinery","Cargo / Ballast Systems","Equipment Related","10.32","Very High","","","Top cover brought in E/R workshop and fabricated","2019-06-21","","Completed","2019-06-15","No","No","No","Internal"]
[null,null,null,null,6197,"48_25/10/2019 2:07:01 PM","2019-05-21","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","T/C air intake room cleaning required.","Miscellaneous","Eng. / Strg. Comp.","Human Error","10.29","Medium","","","Gratings removed, chipped and painted.","2019-07-21","","Completed","2019-06-20","No","No","No","Internal"]
[null,null,null,null,6198,"48_25/10/2019 2:09:27 PM","2019-05-25","Defect","Ship Staff","Suptd. Insp.","COPT#2 Oil caution remark from shore analysis","Cargo Mach.,Deck - Machinery","Cargo / Ballast Systems","Equipment Related","10.7","Medium","","","COPT NO2 OIL SUMP, DRAINED CLEANED AND OIL RENEWED","2019-06-21","","Completed","2019-06-12","No","No","No","Internal"]
[null,null,null,null,6199,"48_25/10/2019 2:12:28 PM","2019-05-25","Defect","Ship Staff","Ship Staff Insp.","Few buttons on MF/HF keypad not functioning . Also,few pins of flat cable connected to the Keypad PCB found damaged making the above mentioned keys inoperational.","Navigation - GMDSS & Communication","Navigation","Equipment Related","4.21","High","","","MF/HF equipment flat cable renewed and tested the GMDSS found working satisfactory.","2019-08-30","STAI195045","Completed","2019-07-18","No","No","No","Internal"]
[null,null,null,null,6200,"48_25/10/2019 2:15:59 PM","2019-05-27","Defect","Ship Staff","Ship Staff Insp.","Soot blower # 3 of LP side is stuck. Not operating","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Soot Blower LP3 removed from place , soot blower was stuck badly, sealing air passage was choked completely, same made free and cleared. Soot blower fitted back in place and tried out , satisfactory","2019-06-30","","Completed","2019-06-29","No","No","No","Internal"]
[null,null,null,null,6201,"48_25/10/2019 2:18:03 PM","2019-05-27","Critical Equipment,Defect","Ship Staff","Ship Staff Insp.","Clutch lining of Vacuum pump of Emergency Fire Pump came off while trying out of the pump","Critical Equip.","Emgcy. Systems","Equipment Related","5.41","Very High","","","Clutch lining renewed with the spare recd , pump tried out, satisfactory","2019-08-30","","Completed","2019-07-26","No","No","No","Internal"]
[null,null,null,null,6202,"48_25/10/2019 2:21:26 PM","2019-05-29","Defect","Ship Staff","Ship Staff Insp.","Vibscanner is not operational","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Received new vibscanner. ","2019-11-30","","Completed","2019-11-07","No","No","No","Internal"]
[null,null,null,null,6203,"48_25/10/2019 2:25:15 PM","2019-06-01","Defect","Ship Staff","Ship Staff Insp.","Siren for wind Hi-Hi alarm not operational and only light is working.","Elect. Mach. & Equip.","Cargo / Ballast Systems","Equipment Related","10.37","Medium","","","Spares received at Singapore on 31/08/2019. Wind Hi-Hi siren and light replaced. Working satsifactorily","2019-10-31","","Completed","2019-09-02","No","No","No","Internal"]
[null,null,null,null,6204,"48_25/10/2019 2:29:07 PM","2019-06-11","Critical Equipment,Defect","Ship Staff","Ship Staff Insp.","The GMT time in the BilgeGuard is 11-12 minutes behind the actual GMT time","Critical Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","CHANGED 15 PPM MONITOR. NOW DIFFERENCE IS 3 MINS","2019-10-30","","Completed","2019-10-12","No","No","No","Internal"]
[null,null,null,null,6205,"48_25/10/2019 2:32:38 PM","2019-06-11","Defect","Ship Staff","Ship Staff Insp.","One of the Personal Gas Meter MSA Altair 4X (Sr no. 06028737) Showing Error message on O2, CO & H2S sensor on starting the equipment","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.23","Very High","","","Replaced with the new gas meter received under warranty at GOLA, US on 09th July 2019","2019-08-30","","Completed","2019-07-09","No","No","No","Internal"]
[null,null,null,null,6206,"48_25/10/2019 2:37:17 PM","2019-06-12","Defect","Ship Staff","Ship Staff Insp.","The WBT gas detection system function giving Fault 19 and 17. and is inoperable. FAULT (19) - “No custom setup, using default setup” comes and later after 15-20 seconds the FAULT(17) – “Analyzing unit no answer” shows.","Critical Equip.,Elect. Mach. & Equip.","Cargo / Ballast Systems","Equipment Related","5.22","High","","","Makers technician attanded vessel at GOLA, US on 08th July 2019. Troubleshooting done, necessary spares changed by technician and reconfiguration done.","2019-08-30","","Completed","2019-07-08","No","No","No","Internal"]
[null,null,null,null,6207,"48_25/10/2019 2:40:16 PM","2019-06-12","Defect","Ship Staff","Ship Staff Insp.","UTI (Sr. No. G17710) showing error message on start up indicating ‘’No msg’’.","Miscellaneous","Cargo / Ballast Systems","Equipment Related","8.12","Medium","","","Tape was unwinded to check for any damage and found tape damage at 60cm mark. Continuity test was done for the UTI to confirm the tape error.As per message from office as vessel have total 4 UTIs, so this faulty UTI to be landed ashore at next","2019-10-31","","Completed","2019-08-03","No","No","No","Internal"]
[null,null,null,null,6208,"48_25/10/2019 2:42:33 PM","2019-06-16","Defect","Ship Staff","Ship Staff Insp.","WBT 1 (P) gauge showing erratic reading","Elect. Mach. & Equip.","Cargo / Ballast Systems","Equipment Related","8.8","Medium","","","Renewed sensor on 02nd Oct 2019.","2019-10-31","","Completed","2019-10-02","No","No","No","Internal"]
[null,null,null,null,6225,"48_25/10/2019 2:44:53 PM","2019-06-20","Defect","Ship Staff","Ship Staff Insp.","Kyma Engine Analyser defective","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Changed the cable connecting to computer by Technician","2019-11-30","","Completed","2019-10-31","No","No","No","Internal"]
[null,null,null,null,6209,"48_25/10/2019 2:47:46 PM","2019-06-21","Defect","Ship Staff","Ship Staff Insp.","The local touch panel of WHRS( EGB) does not operate with touch, however operational with mouse","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.37","Medium","","","The touch screen panel renewed","2019-11-30","","Completed","2019-10-20","No","No","No","Internal"]
[null,null,null,null,6210,"48_25/10/2019 2:56:36 PM","2019-06-24","Defect","Ship Staff","Ship Staff Insp.","HFO PFR P/P NO2 MAGNETIC COUPLING CASING HOLED","E/R - Purifier","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","CHANGED CAN OF THE COUPLING","2019-10-31","","Completed","2019-10-10","No","No","No","Internal"]
[null,null,null,null,6211,"48_25/10/2019 2:59:03 PM","2019-06-29","Defect","Ship Staff","Ship Staff Insp.","KW not matching with KWh meter reading and which leads to high SFOC, diff in % utilization of AEs.Actually KWHR is not for present KW","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.37","Medium","","","RESET THE KWH METER. NOW SHOWING VALUES CORRECTLY","2019-10-31","","Completed","2019-10-15","No","No","No","Internal"]
[null,null,null,null,6212,"48_25/10/2019 3:06:56 PM","2019-07-06","Defect","Ship Staff","Ship Staff Insp.","M/E F.O. leak off alarm not coming in the AMS","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Changed the Net DI 16. found alarm stilll there. Then found that in the tag in the AMS the switch had shifted to Man. Changed back to Auto. It is working fine. Changed it back to old NET DI16. Still it is functional.","2019-09-30","","Completed","2019-09-10","No","No","No","Internal"]
[null,null,null,null,6213,"48_25/10/2019 3:13:00 PM","2019-07-12","Defect","Ship Staff","Ship Staff Insp.","EGB exhasut gas outlet temperature probe giving wrong readings","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","needs replacement. Shall raise RO for same. Entered in DD defect list","2019-09-30","","Completed","2019-09-15","No","No","No","Internal"]
[null,null,null,null,6222,"48_25/10/2019 4:23:34 PM","2019-07-18","Defect","Ship Staff","Ship Staff Insp.","Stbd windlass Hydraulic brake Cylinder leaking from Cylinder top seal during anchoring operations","Deck - Mooring Machinery","Mooring","Equipment Related","9.2","Very High","","","Road seal and scrapper ring renewed. Brake tried out and found satisfactory. No further leaks observed.","2019-08-30","","Completed","2019-08-26","No","No","No","Internal"]
[null,null,null,null,6223,"48_25/10/2019 4:26:54 PM","2019-07-20","Defect","Ship Staff","Ship Staff Insp.","IG 43 - deck isolation valave for the IG Line after the IG NRV was found to be leaking and not holding","Cargo Mach.,Inert Gas","Cargo / Ballast Systems","Equipment Related","8.25","Very High","","","IG 43 valve removed from location and found valve disc damaged. Valve disc was builded and put back in plce again. But still minor leak exist. RO raised for Valve disc and seat ring. Valve renewed.","2019-10-30","STAI190182","Completed","2019-10-25","No","No","No","Internal"]
[null,null,null,null,6214,"48_25/10/2019 3:24:54 PM","2019-07-23","Defect","Ship Staff","Ship Staff Insp.","UTI (Sr. No. G18578) Display becomes blurred everytime after 5-10 minutes of operation","Miscellaneous","Cargo / Ballast Systems","Equipment Related","8.12","Medium","","","Interchanged with the Display unit of UTI G17710 which was to be landed ashore as per message from office. Now UTI G 18578 is in good working order","2019-10-31","","Completed","2019-08-03","No","No","No","Internal"]
[null,null,null,null,6215,"48_25/10/2019 3:35:14 PM","2019-07-23","Defect","Ship Staff","Ship Staff Insp.","Work shop AC OCR under rated ,getting tripped","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.37","Medium","","","Spares received and changed. Found working satisfactory.","2019-10-31","","Completed","2019-10-09","No","No","No","Internal"]
[null,null,null,null,6216,"48_25/10/2019 3:37:27 PM","2019-07-24","Defect","Ship Staff","Ship Staff Insp.","STBD life boat control circuit switch damaged","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.29","High","","","Requisition received at Singapore on 31/08/2019. Control circuit replaced. Working satisfactorily now.","2019-10-15","","Completed","2019-09-03","No","No","No","Internal"]
[null,null,null,null,6217,"48_25/10/2019 3:42:18 PM","2019-07-24","Defect","Ship Staff","Ship Staff Insp.","Two wire programmable TX defective","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Spares received and changed. Found working satisfactory.","2019-10-30","","Completed","2019-09-26","No","No","No","Internal"]
[null,null,null,null,6218,"48_25/10/2019 3:48:02 PM","2019-07-25","Defect","Ship Staff","Ship Staff Insp.","Scrubber p/p mech seal leaking","E/R - Aux. Mach.","Cargo / Ballast Systems","Equipment Related","10.31","Very High","","","Mechanical sal renewed. Pump tried out.","2019-08-15","","Completed","2019-08-08","No","No","No","Internal"]
[null,null,null,null,6219,"48_25/10/2019 3:50:01 PM","2019-08-08","Defect","Ship Staff","Ship Staff Insp.","Cover for General Alarm switch on Port/Stbd boat deck broken","Elect. Mach. & Equip.,LSA / FFA","Safety / LSA / FFA","Equipment Related","10.37","Medium","","","Spares received and changed. Found working satisfactory.","2019-10-31","","Completed","2019-10-11","No","No","No","Internal"]
[null,null,null,null,6220,"48_25/10/2019 3:52:18 PM","2019-08-11","Critical Equipment","Ship Staff","Ship Staff Insp.","The battery for BilgeMon 488 for OWS showing voltage 0.330 V against the required value of 2.5","Critical Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","CHANGED 15 PPM SENSOR WITH NEW","2019-10-31","","Completed","2019-10-12","No","No","No","Internal"]
[null,null,null,null,6221,"48_25/10/2019 3:57:52 PM","2019-08-16","Critical Equipment,Defect","Ship Staff","Ship Staff Insp.","Fire and GS p/p 1 mech seal leaking","Critical Equip.","Eng. / Strg. Comp.","Equipment Related","10.31","Very High","","","Pump dismantled and overhauled, mech seal and bottom line brearing renewed","2019-08-30","","Completed","2019-08-23","No","No","No","Internal"]
[null,null,null,null,9498,"48_10/01/2020 6:35:07 AM","2019-09-09","Observation","Owner / Marine / Tech. Suptd.","Nav Audit / Verification","The actual time of arrival to each waypoint was not mentioned in the way point sheet of the passage plan. The arrival times were recorded in the deck log book. ","Navigation - Others","Navigation","Inappropriate Procedure","","","","","Vessel has sterted writing the actual time of arrival to each waypoint in the way point sheet of the passage plan as well as recording in the deck log book. All the navigating officers have been familiarised with correct procedures of filling the passage plan waypoint sheet.","2019-12-06","","Completed","2019-12-06","No","No","No","Internal"]
[null,null,null,null,9499,"48_10/01/2020 7:39:39 AM","2019-09-09","Observation","Owner / Marine / Tech. Suptd.","ISM Audit","Some of the SOPEP gear items (Shovels, broom) were not marked with the 2 red bands as required by company procedures.","Miscellaneous","MARPOL Related","Inappropriate Procedure","","","","","Shovels, Brooms, Scoops etc which were not having red band were marked with red band as per company procedures. All other items cross checked and found bearing red bands on them. Uncontrolled copy of COMPANY PROCEDURES (12.02.12.00.00) Posted in SOPEP LOCKER for easy reference for ship staff.","2020-12-08","","Completed","2020-12-06","No","No","No","Internal"]
[null,null,null,null,8595,"48_Thu Sep 12 2019 17:43:26 GMT+0000 (Coordinated Universal Time)","2019-09-09","Defect","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","The port and Starboard side hose crane's booms were not fitted with\n\nangle indicator.","Deck - Machinery","General Appearance","Equipment Related","8.5","Very High","","","OPERATORS COMMENTS:\n\nWe wish to inform that the port and stbd side hose handling cranes have a SWL of 20T and this\n\nSWL applies for the full operational range corresponding to maximum and minimum operating\n\nradius / angles, i.e. minimum operating radius of 4.4 meter and maximum operating radius of\n\n20 meter. The crane booms cannot be elevated or lowered to angles greater or lower than the\n\nstated operating radius / angle as the maximum and minimum radius limit is limited /\n\nrestricted by the cylinder’s stroke ends.\n\nSince these hose handling cranes are provided with limit devices for safe operation and the\n\nSWL of the crane is applicable over the whole range, an angle indicator has not been provided\n\nfor the boom by the Crane Maker. Same has been confirmed by the Crane Maker’s.\n\nWe also wish to confirm that the operating radius and SWL is permanently marked on the\n\nboom of these cranes. For ready reference we have attached the relevant pages from the\n\nmaker’s manual of the ship’s hose handling crane.","2019-09-24","","Completed","2019-09-24","No","No","No","External"]
[null,null,null,null,8598,"48_Thu Sep 12 2019 18:25:54 GMT+0000 (Coordinated Universal Time)","2019-10-09","Defect","Owner / Marine / Tech. Suptd.","ISM Audit","Two EEBD pressure found less than 200 bar due inspection","LSA / FFA","Safety / LSA / FFA","Human Error","5.44","High","","","EEBD were refilled to 200 bar pressure. All EEBDS and BA sets were checked to ensure compliance. Concerned officer was briefed to deligently carry out weekly and monthly checks and ensure compliance at all times.","2019-10-15","","Completed","2019-10-09","No","No","No","Internal"]
[null,null,null,null,8599,"48_Thu Sep 12 2019 18:29:30 GMT+0000 (Coordinated Universal Time)","2019-10-09","Defect","Owner / Marine / Tech. Suptd.","MLC Audit","Crew messroom refrigerator door packing damaged and food items kept inside spoilt.","Accommodation","MLC Related","Equipment Related","11.13","Low","","","Door packing was renewed and confirmed door sealing properly. ","2019-10-31","","Completed","2019-10-15","No","No","No","Internal"]
[null,null,null,null,8600,"48_Thu Sep 12 2019 18:33:33 GMT+0000 (Coordinated Universal Time)","2019-10-09","Defect","Owner / Marine / Tech. Suptd.","ISPS Audit","Anchor Hawse pipe cover not secured. ","Deck - Machinery","ISPS Related","Behaviour Based","7.12","High","","","Hawse pipe covers put in place and secured. All personnel briefed regarding Security procedures to be followed and precautions to be taken. Importance of securing hawse pipe covers reiterated to all.","2019-10-15","","Completed","2019-10-09","No","No","No","Internal"]
[null,null,null,null,6147,"48_25/10/2019 3:59:57 PM","2019-10-10","Defect","Ship Staff","Ship Staff Insp.","Grey water discharge pump not taking suction.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Grey water discharge Pump overhauled, mouth ring renewed with spare","2020-02-10","STAI190222","Completed","2020-03-01","No","No","No","Internal","Spares received now. Please complete job ASAP. Target date revised accordingly."]
[null,null,null,null,6148,"48_24/10/2019 11:58:45 PM","2019-10-14","Defect","Ship Staff","Ship Staff Insp.","CCTV -CAMERA NO: 2 (FWD) NOT WORKING , CAMERA NO: 3 ( FUNNEL DECK ) -ERRATIC","Miscellaneous","ISPS Related","Equipment Related","7.6","Medium","","","As per Office instructions Defect to be closed","2020-04-28","","Completed","2020-05-05","No","No","No","Internal","New CCTV installation to be carried out.  Remove the defect from list."]
[null,null,null,null,6244,"48_2019-03-11 07:06:56.000","2019-10-31","Breakdown","Ship Staff","Ship Staff Insp.","Fwd Air horn not working.","Navigation - Others","Navigation","Equipment Related","","","","","Spares received and renewed. Fog horn assembled and now in use","2019-11-30","","Completed","2019-11-11","No","No","No","Internal"]
[null,null,null,null,8594,"48_Mon Mar 11 2019 07:06:56 GMT+0000 (Coordinated Universal Time)","2019-10-31","Breakdown","Ship Staff","Ship Staff Insp.","Fwd Air horn not working.","Navigation - Others","Navigation","Equipment Related","4.7","High","","","Spares received and renewed. Fog horn assembled and now in use","2019-11-30","","Completed","2019-11-11","No","No","No","Internal"]
[null,null,null,null,6145,"48_2019-08-11 19:37:25.000","2019-11-05","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Left over pneumatic pipe of old BWTS system in steering gear room to remove","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","All old pneumatic pipes removed and terminated. ","2019-11-15","","Completed","2019-11-10","No","No","No","External"]
[null,null,null,null,6150,"48_2019-08-11 09:37:39.000","2019-11-05","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Mooring wires are covered with mud due to use in yard. Cleaning and greasing required.","Miscellaneous","Mooring","Equipment Related,External Factors","9.17","High","","","All mooring wires cleaned and greasing carried out. Reported in weekly manitenance report. (DHT Taiga - Deck maintenance Report (16th Dec 2019 - 22nd Dec 2019).xlsx)","2020-02-05","","Completed","2019-12-20","No","No","No","Internal"]
[null,null,null,null,6151,"48_2019-08-11 09:46:40.999","2019-11-05","Defect","Owner / Marine / Tech. Suptd.","Ship Staff Insp.","Various tank domes of WBT and COT has rust weep marks. Derusting and painting required.","Deck - Pipe / Fittings","Cargo / Ballast Systems","External Factors","8.18","High","","","All WBT and COT tank domes derusted and painted with full coat of green paint. Required Stencilling done.","2020-03-01","","Completed","2020-02-25","No","No","No","Internal"]
[null,null,null,null,6152,"48_2019-08-11 10:25:48.000","2019-11-05","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","All the PV valves inspection date stencil to change.","Deck - Pipe / Fittings","General Appearance","Equipment Related","8.21","High","","","stencilling of overhauling date  done on all PV valve.","2019-11-30","","Completed","2019-11-11","No","No","No","Internal"]
[null,null,null,null,6153,"48_2019-08-11 10:29:34.000","2019-11-05","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Outside pump room Stbd side air valve leaking, To be renewed.","Deck - Pipe / Fittings","Eng. / Strg. Comp.","Equipment Related","11.4","Very High","","","air manifold valve  renewed.","2019-11-20","","Completed","2019-11-18","No","No","No","Internal"]
[null,null,null,null,6154,"48_2019-08-11 10:45:11.000","2019-11-05","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Fire line pipe in scrubber room, just above the main power panel vibrates a lot at higher RPM. More supports to be welded.","LSA / FFA","Eng. / Strg. Comp.","External Factors","11.5","Medium","","","Fitted extra supports for pipe lines","2019-11-20","","Completed","2019-11-20","No","No","No","Internal"]
[null,null,null,null,6155,"48_2019-08-11 19:49:28.000","2019-11-05","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","MSDS and PPE to place in BWTS room for neutralizing chemicals.","Cargo Mach.","Cargo / Ballast Systems","Inappropriate Procedure","10.32","Very High","","","MSDS AND PPE placed in location.","2019-11-15","","Completed","2019-11-10","No","No","No","External"]
[null,null,null,null,6156,"48_2019-11-08 19:51:48.999","2019-11-05","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Various electrical insulation mat in E/R and emergency DG room are deteriorated or salt soaked. To be renewed.","Miscellaneous","Eng. / Strg. Comp.","Inappropriate Procedure","11.11","Very High","","","Insulation mats replaced.","2019-11-14","","Completed","2019-11-29","No","No","No","External"]
[null,null,null,null,6157,"48_2019-11-08 20:02:45.000","2019-11-05","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Zebra stripe sticker to put in the newly installed low head pipe in  ER bottom platform","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","External Factors","10.32","Very High","","","Stickers placed in location.","2019-11-12","","Completed","2019-11-17","No","No","No","External"]
[null,null,null,null,6158,"48_2019-11-08 20:13:51.000","2019-11-05","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ME LO auto filter shaft seal leaking. To be renewed","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Seal renewed.","2019-12-20","","Completed","2019-12-13","No","No","No","External",""]
[null,null,null,null,6159,"48_2019-08-11 20:17:42.000","2019-11-05","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Economiser surrounding to clean and paint","Miscellaneous","Eng. / Strg. Comp.","External Factors","10.32","Very High","","","To be painted. Painting completed by 30th Dec 2019","2019-12-31","","Completed","2019-12-30","No","No","No","External","Target date revised in view of busy schedule of the vessel."]
[null,null,null,null,6239,"48_2019-08-11 19:41:53.000","2019-11-05","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Water cooler outside ECR not operational. Cooler Compressor not running.","Miscellaneous","General Appearance","Equipment Related","10.32","Very High","","","Leak rectified and cooler put in use","2019-11-15","","Completed","2019-11-09","No","No","No","Internal"]
[null,null,null,null,6240,"48_2019-11-08 19:58:10.999","2019-11-05","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","T/C suction room door not easy to open. To ease up and grease.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","DOOR EASED UP. ","2019-11-08","","Completed","2019-11-06","No","No","No","External"]
[null,null,null,null,6241,"48_2019-11-08 20:07:39.000","2019-11-05","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Steering gear room door self-closing mechanism needs to adjust as door remains in open condition.","Miscellaneous","Eng. / Strg. Comp.","Inappropriate Procedure","10.32","Very High","","","Door adjusted. ","2019-11-07","","Completed","2019-11-07","No","No","No","External"]
[null,null,null,null,6242,"48_2019-08-11 20:09:57.000","2019-11-05","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Chlorine dosing pump of STP was running but no liquid passing. To be purged and checked regularly.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Checked and purged. ","2019-11-05","","Completed","2019-11-05","No","No","No","External"]
[null,null,null,null,6243,"48_2019-11-08 10:42:57.000","2019-11-05","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Drain near both aft E/R blower are choked. To be cleared.","Miscellaneous","Structural Condn. / WT integrity ","External Factors","6.2","High","","","Drain line opened up for both blowers and cleared. ","2019-12-05","","Completed","2019-11-13","No","No","No","Internal"]
[null,null,null,null,6245,"48_2019-08-11 09:43:02.000","2019-11-05","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Water cooler in officer mess room was kept in isolated condition due to leak. TO be made operational.","Accommodation","MLC Related","Equipment Related","11.13","Low","","","Fountain tap leak was rectified. System back in operation. ","2019-11-19","","Completed","2019-11-14","No","No","No","Internal"]
[null,null,null,null,6246,"48_2019-11-08 19:44:49.998","2019-11-05","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Both boiler gauge glass light not working.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Light changed. ","2019-11-15","","Completed","2019-11-15","No","No","No","Internal"]
[null,null,null,null,6248,"48_43688.8260185185","2019-11-05","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","MSDS and PPE to place in BWTS room for neutralizing chemicals.","Cargo Mach.","Cargo / Ballast Systems","Inappropriate Procedure","10.32","Very High","","","MSDS Put in place in BWTS room for Neutralizer chemicals, Sodium hypochlorite & hydrogen gas.","2019-11-15","","Completed","2019-11-10","No","No","No","External"]
[null,null,null,null,8611,"48_Fri Nov 08 2019 20:13:51 GMT+0000 (Coordinated Universal Time)","2019-11-05","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ME LO auto filter shaft seal leaking. To be renewed","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Will be renewed in the first oppurtunity. L.O. BACKWASH FILTER SERVICE CARRIED OUT. ALL CANDLES REPLACED WITH CLEANED SPARE. TOP X-OIL SEAL(2PCS) REPLACED WITH NEW SPARE.","2019-12-20","","Completed","2019-12-13","No","No","No","External"]
[null,null,null,null,7090,"48_Sun Aug 11 2019 09:37:39 GMT+0000 (Coordinated Universal Time)","2019-11-05","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Mooring wires are covered with mud due to use in yard. Cleaning and greasing required.","Miscellaneous","Mooring","Equipment Related,External Factors","9.17","High","","","Mud cleaning & Greasing of all the 10 mooring wires in fwd carried out. Remaining all 10 ropes in the aft station were thorougly washed of the mud - Greasing was found in good condition on them. Both the fire wires greasing also done.","2020-02-05","","Completed","2019-12-20","No","No","No","Internal"]
[null,null,null,null,7094,"48_Sun Aug 11 2019 10:25:48 GMT+0000 (Coordinated Universal Time)","2019-11-05","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","All the PV valves inspection date stencil to change.","Deck - Pipe / Fittings","General Appearance","Equipment Related","8.21","High","","","Overhauling dates stencilling done on all PV valve.","2019-11-30","","Completed","2019-11-11","No","No","No","Internal"]
[null,null,null,null,7095,"48_Sun Aug 11 2019 10:29:34 GMT+0000 (Coordinated Universal Time)","2019-11-05","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Outside pump room Stbd side air valve leaking, To be renewed.","Deck - Pipe / Fittings","Eng. / Strg. Comp.","Equipment Related","11.4","Very High","","","air manifold valve renewed.","2019-11-20","","Completed","2019-11-18","No","No","No","Internal"]
[null,null,null,null,7096,"48_Sun Aug 11 2019 19:49:28 GMT+0000 (Coordinated Universal Time)","2019-11-05","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","MSDS and PPE to place in BWTS room for neutralizing chemicals.","Cargo Mach.","Cargo / Ballast Systems","Inappropriate Procedure","10.32","Very High","","","MSDS AND PPE put in place in BWTS room","2019-11-15","","Completed","2019-11-10","No","No","No","External"]
[null,null,null,null,7097,"48_Sun Aug 11 2019 10:45:11 GMT+0000 (Coordinated Universal Time)","2019-11-05","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Fire line pipe in scrubber room, just above the main power panel vibrates a lot at higher RPM. More supports to be welded. ","LSA / FFA","Eng. / Strg. Comp.","External Factors","11.5","Medium","","","fitted extra supports on the pipeline.","2019-11-20","","Completed","2019-11-20","No","No","No","Internal"]
[null,null,null,null,7098,"48_Fri Nov 08 2019 20:02:45 GMT+0000 (Coordinated Universal Time)","2019-11-05","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Zebra stripe sticker to put in the newly installed low head pipe in  ER bottom platform","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","External Factors","10.32","Very High","","","Out the stripes stickers. ","2019-11-12","","Completed","2019-11-17","No","No","No","External"]
[null,null,null,null,7099,"48_Fri Nov 08 2019 19:51:48 GMT+0000 (Coordinated Universal Time)","2019-11-05","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Various electrical insulation mat in E/R and emergency DG room are deteriorated or salt soaked. To be renewed.","Miscellaneous","Eng. / Strg. Comp.","Inappropriate Procedure","11.11","Very High","","","REPLACED THE INSULATION MATS","2019-11-14","","Completed","2019-11-29","No","No","No","External"]
[null,null,null,null,6247,"48_16/11/2019 8:59:18 AM","2019-11-14","Guarantee Claim","Ship Staff","Ship Staff Insp.","BWTS filter inlet valves BT-1211 & BT-2211 not operating in remote or Local mode. No power available on the valve actuator display unit because of faulty PCB in the valve actuators.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.14","Very High","","","PCBs renewed and close/Open calibration carried out also new PCB renewed setting done . now valve can be operated from local and remote as well","2020-02-14","","Completed","2020-02-11","No","No","No","Internal","GC spares have been received, will be supplied at next convenient port."]
[null,null,null,null,6149,"48_25/10/2019 3:17:08 PM","2019-11-18","Defect","Ship Staff","Ship Staff Insp.","APK WBT gauge showing erratic reading","Elect. Mach. & Equip.","Cargo / Ballast Systems","Equipment Related","8.12","Medium","","","New level sensor received and fitted. APK WBT guage calibrated and working satisfactory.","2020-02-18","STAI190182","Completed","2020-02-11","No","No","No","Internal","Target date revised as the spares are not yet ready. Please mention correct RO no."]
[null,null,null,null,8605,"48_Mon Dec 09 2019 23:52:54 GMT+0000 (Coordinated Universal Time)","2019-11-19","Defect","Owner / Marine / Tech. Suptd.","Others (Eg. Insurance etc.)","CCR Movement Book - No entry for Line draining sighted after completion of Loading on 18 July 2019 and completion of discharging on 10th Sept 2019. ","Documentation","Cargo / Ballast Systems","Human Error","8.5","Very High","","","Noted, Line draining missed out for writing in the CCR log but please note that Line draining is part of the ''12.80.13.094.00 Completion of cargo & Pre departure checklist'' checklist and it has been filed there. Copy attached.\n\nPreventive action : Discussed with all officers & will ensure line draining enteries and timings to be maintained in CCR log as well.  \n\n","2019-11-30","","Completed","2019-11-30","No","No","No","Internal"]
[null,null,null,null,8606,"48_Thu Sep 12 2019 23:55:21 GMT+0000 (Coordinated Universal Time)","2019-11-19","Defect","Owner / Marine / Tech. Suptd.","Others (Eg. Insurance etc.)","Ship Shore Safety Checklist dated 17 July 2019 Pt 33 - No comment entered in Remarks.","Documentation","Cargo / Ballast Systems","Human Error","5.9","Very High","","","Comment added in point 33. All recent checklists verified that all items are completed properly.Discussed with all officers & will ensure all relevent A items are marked with comments\n\n","2019-11-30","","Completed","2019-11-30","No","No","No","Internal"]
[null,null,null,null,8607,"48_Thu Sep 12 2019 23:57:23 GMT+0000 (Coordinated Universal Time)","2019-11-19","Defect","Owner / Marine / Tech. Suptd.","Others (Eg. Insurance etc.)","No entry for Operational Test of Cargo and ballast hydraulic valves sighted prior Load Port GOLA,US","Documentation","Cargo / Ballast Systems","Behaviour Based,Human Error","8.5","Very High","","","Operational test of cargo and ballast hydraulic valves already written under ''Cargo valves hydraulic system tried out, hydraulic tank level checked'' on page 90 of CCR log. Copy attached & highlighted.\n\nPreventive action : Discussed with all officers & will ensure that all individual valves for ballast & cargo system to be tried out and entry in the CCR log to be written clearly.\n\n","2019-11-30","","Completed","2019-11-30","No","No","No","Internal"]
[null,null,null,null,8608,"48_Tue Dec 10 2019 00:00:24 GMT+0000 (Coordinated Universal Time)","2019-11-19","Defect","Owner / Marine / Tech. Suptd.","Bunkering Audit","Bunker Transfer Plan / Checklist 12.04.08.011.01 Section 7 - Monitoring of H2S/Benzene Vapors : \n\nBenzene reading measured by detector tubes shall be mentioned < Min value that can be measured by the specific tube. For example by Gastec tubes Min measurable value is 0.05 ppm, hence in that case benzene shall be mention <0.05 ppm (if no discoloration observed)\n\nUnderstand vessel has kept the Gas tubes as evidence of monitoring.\n\n","Documentation","Eng. / Strg. Comp.","Human Error","5.9","Very High","","","As per checklist, the Primary System :UHF Ch-2 and Secondary System :VHF Ch-16 and same updated for backup communication system. Copy attached. \n\nDiscussed with all engineer's regarding specifying the communication system established with bunker barge in the checklist properly. \n\n","2019-11-30","","Completed","2019-11-30","No","No","No","Internal"]
[null,null,null,null,8609,"48_Sat Oct 12 2019 00:02:53 GMT+0000 (Coordinated Universal Time)","2019-11-19","Defect","Owner / Marine / Tech. Suptd.","Bunkering Audit","Bunker Safety Checklist for FO dated 06 Nov 2019 - Backup communication system not agreed and remarked in Pt 7 of the checklist. ","Documentation","Eng. / Strg. Comp.","Human Error","5.9","Very High","","","As per checklist, the Primary System :UHF Ch-2 and Secondary System :VHF Ch-16 and same updated for backup communication system. Copy attached. \n\nDiscussed with all engineer's regarding specifying the communication system established with bunker barge in the checklist properly. \n\n","2019-11-30","","Completed","2019-11-30","No","No","No","Internal"]
[null,null,null,null,6146,"48_25/10/2019 2:53:02 PM","2019-11-21","Critical Equipment","Ship Staff","Ship Staff Insp.","Display for OWS Bilge Mon not clear when seen from front, however can be seen at certain angle","Critical Equip.","Eng. / Strg. Comp.","Equipment Related","10.37","Medium","","","Display unit Brightness/contrast settings adjusted as per mail from makers. LCD display clear and bright. ","2020-02-21","STAI190136","Completed","2020-05-29","No","No","No","Internal","Maker analysis with the new display is still awaited. Target date revised."]
[null,null,null,null,8604,"48_Thu Sep 12 2019 23:35:23 GMT+0000 (Coordinated Universal Time)","2019-11-24","Defect","Ship Staff","Nav Audit / Verification","When Gyro compass error is not taken during a watch due to bad weather overast skies , this matter is not entered in the Compass error book.","Documentation","Navigation","Behaviour Based,Human Error","4.9","Medium","","","All duty officers were briefed that there should be atleast 6 entries in the compass error book every day when the vessel is at sea. And Duty officers have started entering the reason for not obtaining compass error evry watch.","2019-11-30","","Completed","2019-11-24","No","No","No","Internal"]
[null,null,null,null,7092,"48_Sun May 12 2019 14:13:21 GMT+0000 (Coordinated Universal Time)","2019-11-25","Defect","Ship Staff","Ship Staff Insp.","Mechanical seal leaking for NO.2 Econimiser feed pump","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","To change the seal. SUPDT. COMMENT NOTED. VSL HAS SPARE SEAL. PLANNED FOR 3rd WEEK DECEMBER DUE TO BUSY SCHEDULE AT BONNY LOAD PORT. Economiser Feed water Pump No 2 overhauled as the mechanical seal was leaking. Pump was found in seized condition as part of mechanical seal carbon was found stuck in the casing. Pump opened up. Impellers were cleaned. Gaskets were changed. New mechanical seal was put along with new bearings. \n\nPump tried out and all found satisfactory.","2019-12-31","","Completed","2019-12-30","No","No","No","Internal","Target date revised due to load port. TO be completed after load port"]
[null,null,null,null,9497,"48_10/01/2020 6:12:13 AM","2019-12-30","Breakdown","Ship Staff","Ship Staff Insp.","BWTS valve BT2213 inside pumproom - valve motor connected with hydraulic oil cylinder got dislodged from actuator which was assembled with four bolts, These bolts may have come loose due to high vibration in pumproom. The gauge glass on hydraulic tank observed assembled in horizontal direction which makes it difficult for staff to gauge the level of oil inisde cylinder.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","Motor fixed back to actuator. Gauge glass turned in vertical position by turning the cylinder. Lost hydraulic oil replenished. Purging of hydraulic lines carried out. Valve calibration carried out. Valve tested and found operating satisfactory from remote control and local control. Cleaning of area around the valve carried out.","2020-01-05","","Completed","2020-01-03","No","No","No","Internal"]
[null,null,null,null,null,"48_10/1/2020 10:17:47 AM","2020-01-03","Defect","Ship Staff","Ship Staff Insp.","Tube light fittings all around Vsl converted wrongly to LED fittment, without disconnecting choke/ ballast, capacitor.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related",null,null,"Not Applicable","Not Applicable","Changed all tubelights to LED along with wiring.","2020-12-31",null,"Completed","2020-12-17","No",null,null,"Internal"]
[null,null,null,null,9926,"48_20/1/2020 5:57:04 PM","2020-01-19","Guarantee Claim","Ship Staff","Ship Staff Insp.","Sea water temperature sensor faulty. (TE-1111) ","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.12","Medium","","","Sensor renewed with new spare received under GC. Temperature sensor working in order.","2020-02-28","BWTS GC - 001/2020","Completed","2020-03-05","No","No","No","Internal"]
[null,null,null,null,9927,"48_20/1/2020 6:04:25 PM","2020-01-19","Guarantee Claim","Ship Staff","Ship Staff Insp.","BWTS filter inlet valves BT-2211 not closing from local control. Suspect the switch in the local faulty or some function of PCB not responding","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.14","Very High","","","After changing the PCB,Close and Open calibration carried out and new PCB change settings done, now the valve is working from remote and local as well","2020-02-28","","Completed","2020-02-12","No","No","No","Internal"]
[null,null,null,null,10174,"48_27/01/2020 7:20:58 PM","2020-01-20","Defect","Ship Staff","Ship Staff Insp.","The air pressure regulator valve for ME Autobackwash filter faulty","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","As there was lack of spare, the air pressure regulator from Gas detection system was used. Job was completed and now its working fine","2020-01-21","","Completed","2020-01-20","No","No","No","Internal"]
[null,null,null,null,10523,"48_03/02/2020 19:21:47","2020-01-25","Defect","Ship Staff","Ship Staff Insp.","2P HFO bunker tnak Heating coil steam return line leaking from flange gasket after the return valve","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Flange gasket to be renewed after closing the main steam valve .","2020-02-01","","Completed","2020-02-01","No","No","No","Internal"]
[null,null,null,null,10524,"48_10/02/2020 7:12:35 PM","2020-01-27","Defect","Ship Staff","Ship Staff Insp.","FPK TANK VENT – During routine inspection of WBT vent heads, observed Float plate top tube type fitting missing (2 Nos. - Port & stbd side vent heads) from float due to which the floats were lying tilted on the support stud and eventually vent lost functionality.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","11.7","High","","","Float guide tube fabricated in e/room workshop for both the floats and welded on the floats. Both the floats fixed back on the vent heads. The support nut inside the vent head have fixed height, so height cannot be adjusted. Both the floats after repair tested for proper functioning and found operating satisfactory.","2020-02-05","","Completed","2020-02-03","No","No","No","Internal"]
[null,null,null,null,10512,"48_10/02/2020 7:37:42 PM","2020-02-01","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Paint failure noticed at few places on deck","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.3","Medium","",""," Paint failure near aft and forward  mooring winches attended. Job completed.","2020-04-01","","Completed","2020-04-01","No","No","No","Internal"]
[null,null,null,null,10513,"48_8/2/2020 10:54:45 AM","2020-02-01","Defect","Owner / Marine / Tech. Suptd.","Ship Staff Insp.","Galley drain pipe stbd side has soft patch to repair","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","External Factors","10.31","Very High","","","Pipe removed and hotwork carried out in ER workshop. Pipe fitted back and No leaks from the line. Working in order.","2020-02-29","","Completed","2020-02-17","No","No","No","Internal"]
[null,null,null,null,10514,"48_8/2/2020 10:57:56 AM","2020-02-01","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","HP drum feed water valve leaking from gland, to repair","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","New valve received renewed and no leaks from the valve.","2020-03-15","","Completed","2020-03-29","No","No","No","Internal","What is RO no of the ordered valve?"]
[null,null,null,null,10515,"48_15/02/2020 12:16:29 AM","2020-02-01","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Workshop entrance door is in bent condition. To repair or to order new. Door of spare part room has its lock knob broken. To renew","Miscellaneous","Eng. / Strg. Comp.","External Factors","","","","","New door received at Singapore on 04 June 2020 and replaced .","2020-04-29","STAI200063","Completed","2020-06-05","No","No","No","Internal","Doors are ready in Singapore and will be supplied at next call Singapore."]
[null,null,null,null,10516,"48_15/02/2020 12:21:41 AM","2020-02-01","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Various markings from yard is still not painted off in engine room","Miscellaneous","Eng. / Strg. Comp.","External Factors","","","","","Markings are painted off/wiped clean.","2020-03-31","","Completed","2020-03-25","No","No","No","Internal"]
[null,null,null,null,10517,"48_15/02/2020 12:26:36 AM","2020-02-01","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Cracked light cover in pump room to renew","Elect. Mach. & Equip.","Cargo / Ballast Systems","Equipment Related","11.11","Very High","","","all cracked light fittings renewed with LED conversion.","2020-03-15","","Completed","2020-03-23","No","No","No","Internal"]
[null,null,null,null,10518,"48_15/02/2020 12:30:50 AM","2020-02-01","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","All engine room blower mushroom vent to de-rust and paint\t","E/R - Aux. Mach.","General Appearance","Equipment Related","","","","","e/r blower derusting and full coat painting completed","2020-03-31","","Completed","2020-03-20","No","No","No","Internal"]
[null,null,null,null,10519,"48_15/02/2020 12:34:07 AM","2020-02-01","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Both lifeboat motor and related area to derust and paint","Hull & Tanks","General Appearance","External Factors","","","","","Derusted and painted areas near lifeboat motor oil tank and related areas.Reported to office in weekly workdone report with photos","2020-02-20","","Completed","2020-02-20","No","No","No","Internal"]
[null,null,null,null,10520,"48_15/02/2020 12:37:06 AM","2020-02-01","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Removed spare VCU and fuel pump to overhaul","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Spare VCU overhauled and ME fuel pump overhauled with new plunger barell and o-rings. Both marked and kept as standby ","2020-02-29","","Completed","2020-03-13","No","No","No","Internal"]
[null,null,null,null,10521,"48_15/02/2020 12:39:02 AM","2020-02-01","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","EGB casing and area cleaning\t","Miscellaneous","General Appearance","External Factors","10.29","Medium","","","Cosmetic upgradation Completed . Area cleaned and painted after receiving the paints.","2020-03-01","","Completed","2020-04-13","No","No","No","Internal","It is long pending job, when it expected to complete."]
[null,null,null,null,10522,"48_15/02/2020 12:42:53 AM","2020-02-01","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Aft deck below scrubber house needs to hydroblast and paint\t","Hull & Tanks","General Appearance","External Factors","11.3","Medium","","","Hydroblasted and full area beneath EGS unit painted with antiskid surface.","2020-03-20","","Completed","2020-03-14","No","No","No","Internal"]
[null,null,null,null,10525,"48_8/2/2020 11:00:47 AM","2020-02-01","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Emergency DG room fuel filter leaking, oil collected below it. To rectify\t\t","Critical Equip.","Emgcy. Systems","Equipment Related","10.35","Very High","","","Filter drain tightened and leak rectified","2020-02-05","","Completed","2020-02-04","No","No","No","Internal"]
[null,null,null,null,10526,"48_8/2/2020 11:03:10 AM","2020-02-01","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","In EGCS room slight SW leak from one of the flange. \t","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Tightened bolts of flanges. ","2020-02-10","","Completed","2020-02-05","No","No","No","Internal"]
[null,null,null,null,10527,"48_15/02/2020 12:32:36 AM","2020-02-01","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Boiler safety valve flange not covered with lagging\t","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","New lagging fabricated and flanges covered up","2020-02-07","","Completed","2020-02-05","No","No","No","Internal"]
[null,null,null,null,10528,"48_15/02/2020 12:19:29 AM","2020-02-01","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Sewage treatment plant chlorine pump in running condition but there is no flow of liquid. Flow indicator dirty and float is not visible\t","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Chlorine pump primed and operation checked and verified. Flow indicator cleaned. Sewage plant working in order","2020-02-10","","Completed","2020-02-03","No","No","No","Internal"]
[null,null,null,null,10529,"48_15/02/2020 12:41:19 AM","2020-02-01","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Save all of bilge tank, hot well to clean. Vent heads needs cleaning","Hull & Tanks","General Appearance","Inappropriate Procedure","11.7","High","","","Save all cleaned and painted. All vents heads inspected, cleaned and painted.","2020-02-04","","Completed","2020-02-04","No","No","No","Internal"]
[null,null,null,null,10530,"48_15/02/2020 12:44:33 AM","2020-02-01","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Steering gear room aft bilges to mark yellow\t","Miscellaneous","Eng. / Strg. Comp.","Inappropriate Procedure","10.32","Very High","","","Bilges marked yellow ","2020-02-07","","Completed","2020-02-04","No","No","No","Internal"]
[null,null,null,null,10531,"48_15/02/2020 12:28:33 AM","2020-02-01","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Foam pump has leakage marks. To be checked while running and seals to renew if required\t","LSA / FFA","Safety / LSA / FFA","Equipment Related","10.29","Medium","","","Mechanical seal renewed and pump tried out no leaks","2020-02-10","","Completed","2020-02-15","No","No","No","Internal"]
[null,null,null,null,10532,"48_15/02/2020 12:23:49 AM","2020-02-01","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Steam ballast pump to overhaul as same is leaking from seal\t","Deck - Machinery","Eng. / Strg. Comp.","Equipment Related","10.31","Very High","","","Mechanical seal of ballast pump renewed , pump tried out no leaks","2020-02-15","","Completed","2020-02-15","No","No","No","Internal"]
[null,null,null,null,10743,"48_3/3/2020 6:16:25 PM","2020-02-15","Defect","Ship Staff","Ship Staff Insp.","Drain line from IGS scrubber tower found to have hole and water leaking\t\t","Inert Gas","Eng. / Strg. Comp.","Equipment Related","","","","","Hot work carried out after permission from office. Drain pipe with flange fabricated and welded. ","2020-02-25","","Completed","2020-02-18","No","No","No","Internal"]
[null,null,null,null,10749,"48_4/3/2020 10:39:17 AM","2020-02-15","Defect","Ship Staff","Ship Staff Insp.","IGS scrubber tower drain pipe leak to rectify.","Inert Gas","Eng. / Strg. Comp.","Equipment Related","","","","","Leak from drain pipe rectified with hotwork after office approval.  New pipe welded as the old pipe found to have corroded badly. New pipe after welding coated with epoxy. Scrubber system tried out no leaks observed.","2020-02-29","","Completed","2020-02-18","No","No","No","Internal"]
[null,null,null,null,10744,"48_3/3/2020 6:20:13 PM","2020-02-21","Defect","Ship Staff","Ship Staff Insp.","Sewage treatment plant Air Blower #2 tripping on overload.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Sewage plant air blower #2 overhauled, found driving end bearing seized. Both end bearing renewed and tried out. Working satisfactory.","2020-02-29","","Completed","2020-02-22","No","No","No","Internal"]
[null,null,null,null,10750,"48_4/3/2020 10:45:10 AM","2020-02-21","Defect","Ship Staff","Ship Staff Insp.","Sewage treatment plant no:2 air blower found to trip on overload.\t","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","No:2 air blower motor driving end bearing found to be seized. Both end bearings renewed and tried out. working in order.","2020-02-29","","Completed","2020-02-22","No","No","No","Internal"]
[null,null,null,null,10741,"48_01/03/2020 6:00:37 PM","2020-02-25","Breakdown,Defect","Ship Staff","Ship Staff Insp.","Two UTIs onboard has developed following errors: -\tUTI # G17710: LED display stopped working. Unable to see temperature readings. Last shore calibration of UTI: 07-Jan-2020. - UTI # 66433 : Temperature readings showing difference of more than 3 deg C and sometimes even more than other UTIs & thermometer. Last shore calibration of UTI: 05-Oct-2019.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.12","Medium","","","Two new UTIs with shore calibration received on 04-Mar-2020 at Singapore EOPL. UTI #17927 & 17928 (Shore calibration date: 27-Feb-2020). Both UTIs tested and found suitable for vessel use.","2020-03-10","STAI205021","Completed","2020-03-04","No","No","No","Internal","already supplied passing Singapore."]
[null,null,null,null,10747,"48_04/03/2020 21:12:33","2020-02-25","Breakdown","Ship Staff","Ship Staff Insp.","Two UTIs onboardhas devolopedfollowing errors:UTI#G17710:LED display stopped working.Unable to see temperature readings.Last shore calibration of UTI07 Jan 2020-UTI #66433","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","Two new UTIs with shore calibration received on 04-Mar-2020 at Singapore EOPL. UTI #17927 & 17928 (Shore calibration date: 27-Feb-2020). Both UTIs tested and found suitable for vessel use.","2020-03-10","STAI205021","Completed","2020-03-04","No","No","No","Internal"]
[null,null,null,null,10742,"48_03/03/2020 3:11:00 PM","2020-02-28","Defect","Ship Staff","Ship Staff Insp.","4P & 5S WBT Level gauges faulty","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","Same defect was duplicated. ","2020-05-01","STAI200080","Completed","2020-02-28","No","No","No","Internal","Awaiting  readiness of spares."]
[null,null,null,null,10837,"48_15/03/2020 3:40:49 PM","2020-03-07","Defect","Ship Staff","Ship Staff Insp.","HP drum PORT water level guage glass  leaking","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","HP drum water level guage glass overhauled. New glass and gaskets changed. No leaks observed","2020-03-15","","Completed","2020-03-08","No","No","No","Internal"]
[null,null,null,null,10836,"48_15/03/2020 3:44:08 PM","2020-03-11","Defect","Ship Staff","Ship Staff Insp.","Inert gas Generator system gas outlet digital temperature indicator faulty","Inert Gas","Eng. / Strg. Comp.","Equipment Related","","","","","New Spare digital indicator received atSingapore on 04 June 2020 and replaced now working ok.","2020-06-11","STAI200082","Completed","2020-06-05","No","No","No","Internal","Awaiting readiness."]
[null,null,null,null,11454,"48_31/3/2020 11:56:39 PM","2020-03-20","Defect","Ship Staff","Ship Staff Insp.","Main Engine Waste gate for exhaust manifold solenoid valve not operational.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","New spare solenoid valve received at Singapore on 04 june 2020 and defective one replaced with new spare . now working ok.","2020-06-30","STAI200075","Completed","2020-06-13","No","No","No","Internal","Will be ready by 5th June 20"]
[null,null,null,null,11453,"48_9/4/2020 7:57:07 AM","2020-03-26","Defect","Ship Staff","Ship Staff Insp.","ECR AC #1 fan abnormal noise & vibrations","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","New blower received at singapore on 10th july and fitted back. Tried our working satisfactory.","2020-05-31","STAI200092","Completed","2020-07-13","No","No","No","Internal"]
[null,null,null,null,null,"48_Sun May 12 2019 14:15:56 GMT+0000 (Coordinated Universal Time)","2020-03-26","Defect","Ship Staff","Ship Staff Insp.","The slewing limit valve for STBD provision crane is defective and broken.","Deck - Machinery","Eng. / Strg. Comp.","External Factors",8.5,"Very High","Not Applicable","Not Applicable","change the spare limit switch. tried out.","2020-09-30","STAI200148","Completed","2020-10-08","No",null,null,"Internal"]
[null,null,null,null,11455,"48_31/3/2020 11:51:13 PM","2020-03-29","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Spare parts inventory to update in PAL\t","Miscellaneous","Eng. / Strg. Comp.","Knowledge Based","","","","","\n\n\n\nSpare part inventory updated","2020-06-30","","Completed","2020-06-28","No","No","No","Internal"]
[null,null,null,null,11456,"48_17/4/2020 5:01:47 AM","2020-04-12","Defect","Ship Staff","Ship Staff Insp.","No.2 Ejector pump for FWG Mech. seal found leaking and pump found to be fitted in reverse direction . Suction /Discharge orientation wrong in last dry dock","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","","","","","Pump overhauled and mech seal renewed ,all clearances taken . Pump installed in right direction and suction /Discharge pipe modification  carried out. Pump tried out and FWG running satisfactory.","2020-04-20","","Completed","2020-04-15","No","No","No","Internal"]
[null,null,null,null,11520,"48_01/05/2020 3:45:16 AM","2020-04-20","Observation","Ship Staff","Ship Staff Insp.","Steam Leak from condensate return pipe at ER 3rd Deck to be rectified.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Steam leaks rectified, flange gaskets renewed.","2020-05-08","","Completed","2020-05-03","No","No","No","Internal"]
[null,null,null,null,11521,"48_01/05/2020 3:49:19 AM","2020-04-22","Defect","Ship Staff","Ship Staff Insp.","Steering gear room vacuum toilet unit not working\t","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","vacuum toilet unit overhauled missing parts replaced with new spare. tried out working satisfactory Spare received @ Singapore on 10th July 2020.","2020-05-31","STAI200110","Completed","2020-07-16","No","No","No","Internal"]
[null,null,null,null,11844,"48_14/05/2020 3:38:38 AM","2020-04-25","Critical Equipment","Ship Staff","Ship Staff Insp.","MF/HF unit is not transmitting DSC Test Alerts with coast stations and other ships","Navigation - GMDSS & Communication","Communication","Equipment Related","4.24","High","","","Complete MF/HF Unit replaced with Upgraded one ( Latest Version)  at Singapore on 11 July 2020.","2020-06-12","","Completed","2020-07-11","No","No","No","Internal","Service being arranged in Tianjin."]
[null,null,null,null,11845,"48_14/05/2020 3:46:15 AM","2020-04-25","Critical Equipment","Ship Staff","Ship Staff Insp.","Aft transducer unit is not relaying signals to echosunder display unit on bridge","Navigation - Echo Sounder / Speed Log","Navigation","Equipment Related","4.7","High","","","Aft transducer sensor with cable renewed at Singapore on 11 July 2020. now working ok ","2020-06-12","","Completed","2020-07-11","No","No","No","Internal"]
[null,null,null,null,13183,"48_05/07/2020 10:51:05 AM","2020-05-12","Defect","Ship Staff","Ship Staff Insp.","FPK TANK VENT – During routine inspection of WBT vent heads, observed Float plate top tube type fitting missing (2 Nos. - Port & stbd side vent heads) from float due to which the floats were lying tilted on the support stud and eventually vent lost functionality.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","11.7","High","","","FP WBT float replaced 2nos with new floats received onboard at Singapore. FPT vesnt in good working condition ","2020-08-31","STAI200124","Completed","2020-08-11","No","No","No","Internal","Correct size vent already supplied. Fit ASAP."]
[null,null,null,null,12018,"48_19/05/2020 20:02:49","2020-05-19","Defect","Ship Staff","Ship Staff Insp.","Port life boat Alarm and Indicating Buzzer defective and not Operational.","LSA / FFA","Emgcy. Systems","Equipment Related","","","","","New spare Buzzer received at Singapore on 04 June 2020 , defective buzzer replaced with new spare received and now working ok","2020-06-05","STAI200122","Completed","2020-06-05","No","No","No","Internal"]
[null,null,null,null,null,"48_04/03/2020 21:17:43","2020-05-26","Defect","Ship Staff","Ship Staff Insp.","4P & 5S WBT Tank radar remote level gauges Faulty","Hull & Tanks","Cargo / Ballast Systems","Equipment Related",null,null,"Not Applicable","Not Applicable","Spares reveived & 4P, 5S WBT sensors replaced with new sensor supplied at Singapore on 15 Oct 2020. System working satisfactorily","2021-01-30","STAI200080","Completed","2020-10-16","No",null,null,"Internal"]
[null,null,null,null,12999,"48_03/07/2020 21:00:45","2020-06-22","Defect","Ship Staff","Ship Staff Insp.","Aft hydraulic mooring winch oil return pipe leaking as pipe found corroded and wasted ","Deck - Mooring Machinery","Mooring","Equipment Related","","","","","After departure pipe removed and new pipe fabricated and fitted back , tried out found ok","2020-06-25","","Completed","2020-06-24","No","No","No","Internal"]
[null,null,null,null,13184,"48_05/07/2020 12:24:02 PM","2020-07-01","Defect","Ship Staff","Ship Staff Insp.","During recent discharging operations at Qingdao and Tianjin, following centre tanks COW machines found not working during \n\n\n\n1C- Nos. 1, 2 & 4 / 2C - nos. 1, 2, & 4 / 3C- No.4 / 4C - No.3 / 5C - Nos. 1, 2, 3 & 4. Oil was passing through these machines but they were not rotating. Follow up on status of COW machines carried out during discharging at Ningbo, China.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.34","High","","","Complete overhaul of COW machines carried out. 1C: TC10, 2C: TC22, 5C: TC53.\n\nMachines tested by turning with allen key, found in good working condition.\n\nLower magnet found damaged due to scratch marks, same replaced. \n\n","2020-09-01","","Completed","2020-09-08","No","No","No","Internal","Understand all COW machine except 3 are ok and overhauling of 3 are in progress. target date revised accordingly."]
[null,null,null,null,13194,"48_16/7/2020 12:25:00 PM","2020-07-03","Defect","Ship Staff","Ship Staff Insp.","Port waste water pipe before storm valve found pinhole on on side near storm valve.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Pipe dismantled and repaired. Painted with epoxy primer paint and fitted back in place. Tested found no leak.","2020-07-11","","Completed","2020-07-11","No","No","No","Internal"]
[null,null,null,null,13195,"48_16/7/2020 12:39:23 PM","2020-07-05","Defect","Ship Staff","Ship Staff Insp.","Waste water overboard valve gasket leaking on the outboard side of storm valve.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Gasket replaced with new one after divers plugged the line. tested no leak.","2020-07-11","","Completed","2020-07-11","No","No","No","Internal"]
[null,null,null,null,13196,"48_16/7/2020 12:47:09 PM","2020-07-06","Defect","Ship Staff","Ship Staff Insp.","Port waste water overboard valve found not holding, suspected storm valve damaged","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Valve replaced with new spare after the divers plugged the line. Tested and no leak","2020-07-11","","Completed","2020-07-11","No","No","No","Internal"]
[null,null,null,null,13182,"48_17/07/2020 10:04:46 AM","2020-07-10","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Stencil the certificate no on both chain stopper and punch mark it for its permanency.","Deck - Mooring Machinery","General Appearance","Equipment Related","","","","","Permanent Beed welded certificate already exists on chain stoppers. Certificate number stencilled on both the chain stoppers","2020-07-31","","Completed","2020-07-20","No","No","No","Internal"]
[null,null,null,null,13186,"48_17/07/2020 9:58:55 AM","2020-07-10","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Insulation sleeve of Sound receptacle in fore peak store is damaged. Sleeve to renew.","Navigation - GMDSS & Communication","General Appearance","Equipment Related","","","","","Sleeve renewed.","2020-07-29","","Completed","2020-07-21","No","No","No","Internal"]
[null,null,null,null,13187,"48_17/07/2020 10:00:36 AM","2020-07-10","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Provision cranes boom derusting and painting to be carried out.","Deck - Machinery","General Appearance","Equipment Related","","","","","Derusting & full coat painting of P & S Provision crane completed.","2020-08-25","","Completed","2020-09-03","No","No","No","Internal","Target date revised as requested."]
[null,null,null,null,13188,"48_16/7/2020 12:59:46 PM","2020-07-14","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Many of the number keys of emergency DG room phone is missing","Miscellaneous","Safety / LSA / FFA","Equipment Related","","","","","Phone numbers keys replaced with new spare.","2020-08-31","STAI200102","Completed","2020-08-27","No","No","No","Internal","Spares will be supplied at next opportunity. Target date revised."]
[null,null,null,null,13189,"48_16/7/2020 1:05:07 PM","2020-07-14","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ME Cylinder heads needs to clean. There are various dry oil marks and dried salt marks present on almost all cylinder heads.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Main engine all Cylinder covers buffed and cleaned ..","2020-08-30","","Completed","2020-07-21","No","No","No","Internal"]
[null,null,null,null,13190,"48_16/7/2020 1:17:08 PM","2020-07-14","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","There is no coupling pad in spider coupling fitted between the propeller shaft and lifeboat engine","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","Coupling pad fabricated and fitted tried out found working ok.","2020-08-30","","Completed","2020-07-19","No","No","No","Internal"]
[null,null,null,null,13191,"48_16/7/2020 1:23:44 PM","2020-07-14","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Various alarm related to ACONIS were active in AMS since June and no investigation has been carried out for same.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","All alarms attended & rectified.","2020-09-30","","Completed","2020-09-18","No","No","No","Internal","Please restart Aconis Pc once vessel is at anchorage and EGCS stopped. Target date revised."]
[null,null,null,null,13192,"48_16/7/2020 1:31:13 PM","2020-07-14","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Workshop air con was not yet operational, even though new air con blower has already been supplied.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","Blower replaced with new spare recieved in singapore.","2020-09-30","STAI200174","Completed","2020-09-08","No","No","No","Internal","Replacement blower  is being arranged."]
[null,null,null,null,13193,"48_16/7/2020 1:10:47 PM","2020-07-14","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Port ECR air con blower making abnormal sound.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","Port ECR air con blower renewed with new spare blower recived in Singapore.","2020-09-30","STAI200174","Completed","2020-09-08","No","No","No","Internal","Will be supplied next call Singapore."]
[null,null,null,null,13197,"48_16/7/2020 12:54:49 PM","2020-07-14","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Steering Gear room drain valve (spring loaded) in engine room found to be seized","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Valve dismantled and overhauled and make it operational.","2020-07-20","","Completed","2020-07-16","No","No","No","Internal"]
[null,null,null,null,13198,"48_16/7/2020 1:26:54 PM","2020-07-14","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Echo sounder aft transducer cable was laid externally by service engineers and hence the manhole door of void space was kept open.  ","Navigation - Echo Sounder / Speed Log","Eng. / Strg. Comp.","Inappropriate Procedure","","","","","The laid through the Conduit pipe and Manhole door secured .","2020-07-20","","Completed","2020-07-17","No","No","No","Internal"]
[null,null,null,null,13331,"48_01/08/2020 23:14:09","2020-07-31","Defect","Ship Staff","Ship Staff Insp.","Aft peak BWTS system flow control valve FCV-3211 showing sensor failure and malfunctioning.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","Received spare PCB against GC. Changed the spare. tried out working fine.","2020-08-31","","Completed","2020-08-13","No","No","No","Internal"]
[null,null,null,null,13332,"48_01/08/2020 23:23:20","2020-07-31","Defect","Ship Staff","Ship Staff Insp.","IG no.2 Blower discharge valve not closing properly .suspecting valve seat ring damage or excessive carbon deposite on the valve seat /valve","Inert Gas","Eng. / Strg. Comp.","Equipment Related","","","","","VALVE OPENED UP, FOUND DISC WAS HALF OPENED. VALVE SEAT WAS INTACTT. ADJUSTED THE ACTUATOR POSITION. TRIED OUT WORKING FINE","2020-08-31","STAI200170","Completed","2020-08-10","No","No","No","Internal","Open the valve and  clear off soot."]
[null,null,null,null,13534,"48_18/8/2020 2:49:21 PM","2020-08-02","Defect","Ship Staff","Ship Staff Insp.","AUX ENGINE GIVING HIGH TEMP. FOR T/C INLET","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Turbo charger nozzle ring replaced with new spare recived in singapore. Aux DG working satisfactory.","2020-10-02","STAI205058","Completed","2020-09-09","No","No","No","Internal","Please renew the nozzle ring."]
[null,null,null,null,13536,"48_19/8/2020 10:58:08 AM","2020-08-02","Defect","Ship Staff","Ship Staff Insp.","EGB drain line valve not holding","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","CHANGED VALVE.","2020-10-02","","Completed","2020-09-02","No","No","No","Internal","Mention the RO number."]
[null,null,null,null,13537,"48_20/08/2020 8:13:50 AM","2020-08-02","Observation","Ship Staff","Ship Staff Insp.","AFT draft gauge in CCR is not operational. Feed to SAAB system in CCR is also showing \"zero\" Reading.","Miscellaneous","Cargo / Ballast Systems","Equipment Related","","","","","PCB card for aft draft gauge replaced with old(used) card available onboard, SPAN & ZERO Calibration of FAT draft gauge sensor carried out at Ningbo anchorage & found operating in satisfactory condition. ","2020-09-30","","Completed","2020-08-26","No","No","No","Internal"]
[null,null,null,null,null,"48_18/8/2020 2:53:24 PM","2020-08-02","Breakdown","Ship Staff","Ship Staff Insp.","MDO FLUSHING PUMP FOR D/G NOT BUILDING PRESSURE AND LEAKING FORM THE MECHANICAL SEAL","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related",null,null,"Not Applicable","Not Applicable","CHANGED PUMP. TRIED OUT. WOKRING SATIS","2021-01-03","STAI 200065","Completed","2020-10-15","No",null,null,"Internal"]
[null,null,null,null,13539,"48_19/08/2020 4:27:15 PM","2020-08-08","Observation","Ship Staff","Ship Staff Insp.","Cooling water line for Hydraulic motor power pack for forward station found leaking.","Deck - Mooring Machinery","Mooring","Equipment Related","","","","","Leaking cooling water pipe fabricated onboard & replaced with leaking cooling water pipe","2020-08-17","","Completed","2020-08-15","No","No","No","Internal"]
[null,null,null,null,13540,"48_19/08/2020 4:23:13 PM","2020-08-12","Observation","Ship Staff","Ship Staff Insp.","Hydraulic oil observed leaking from mooring winch M4  return line.","Deck - Mooring Machinery","Mooring","Equipment Related","11.4","Very High","","","Leaking hydraulic oil pipe fabricated onboard & installed.","2020-08-17","","Completed","2020-08-17","No","No","No","Internal"]
[null,null,null,null,null,"48_19/08/2020 6:24:33 PM","2020-08-18","Defect","Ship Staff","Ship Staff Insp.","ODME Sampling pump inlet side coupling found leaking during quarterly testing of ODME. Gasket, Check valve & guide found badly damaged ","Miscellaneous","Cargo / Ballast Systems","Equipment Related",6.13,"Low","Not Applicable","Not Applicable","Spares received at Singapore on 15 Oct 2020 & replaced. No leakage observed in the flange.","2021-01-20","STAI200197","Completed","2020-10-17","No",null,null,"Internal"]
[null,null,null,null,null,"48_31/08/2020 3:18:41 PM","2020-08-24","Observation","Ship Staff","Ship Staff Insp.","Entrance hatch coaming of WBT 1P, 1S, 2S, 4P, 4S rusted & requires maintenance","Hull & Tanks","General Appearance","External Factors",8.59,"High","Not Applicable","Not Applicable","Derusting & painting of WBT entrance hatch carried out of all WBT's. Pictures sent in weekly work done report.","2020-11-23",null,"Completed","2020-10-10","No",null,null,"Internal"]
[null,null,null,null,13879,"48_30/08/2020 10:40:09 AM","2020-08-26","Observation","Ship Staff","Ship Staff Insp.","Bridge front window No.3 wiper not operational due to broken Belt","Elect. Mach. & Equip.","Navigation","Equipment Related","12.1","High","","","Belt for window wiper motor renewed with new spare received on 6 Sep 2020 at Singapore","2020-10-31","STAI200176","Completed","2020-09-14","No","No","No","Internal","already supplied."]
[null,null,null,null,null,"48_29/8/2020 9:57:38 AM","2020-08-29","Defect","Ship Staff","Ship Staff Insp.","Galley Baking Oven Low insulation 440 volts From heating coils.","Accommodation","General Appearance","Equipment Related",null,null,"Not Applicable","Not Applicable","Heating coils replaced.","2020-12-30","STAI200201","Completed","2020-10-15","No",null,null,"Internal"]
[null,null,null,null,null,"48_15/9/2020 2:46:18 PM","2020-09-01","Defect","Ship Staff","Ship Staff Insp.","Kyma computer in ECR not showing aft draft level and log speed.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related",null,null,"Not Applicable","Not Applicable","Receivd spare isolator . Same changed in the panel on the bridge. Tried out. working fine","2021-01-01",null,"Completed","2020-11-16","No",null,null,"Internal"]
[null,null,null,null,14006,"48_17/09/2020 1:30:32 PM","2020-09-06","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Pump room hatch found with leak stain marks at port side.","Miscellaneous","General Appearance","External Factors","","","","","Derusting & painting of Hatch coaming to be done.","2020-11-30","","Completed","2020-09-25","No","No","No","Internal"]
[null,null,null,null,14009,"48_15/9/2020 2:35:44 PM","2020-09-06","Observation","Owner / Marine / Tech. Suptd.","Engineering Audit","ME turbocharger air suction room to derust and paint","E/R - Aux. Mach.","General Appearance","Equipment Related","","","","","Dresuted . Grit blasted the grating and railing by bringing outside on the Sunken deck. Painted the  grating and the frames and the floor ","2020-10-06","","Completed","2020-09-21","No","No","No","Internal"]
[null,null,null,null,14013,"48_15/09/2020 11:24:22 AM","2020-09-06","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","BWTS Line near the expansion tank covered with salt, it appears while operation it leaks","E/R - Pipes/ valves & fittings","Cargo / Ballast Systems","Equipment Related","","","","","Couplings tighten for BWTS NA line & general cleaning carried out.","2020-09-16","","Completed","2020-09-13","No","No","No","Internal"]
[null,null,null,null,14014,"48_15/09/2020 11:47:15 AM","2020-09-06","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Engine room blower casing rust weep marks appearing. To paint or clean using oxalic acid","E/R - Pipes/ valves & fittings","General Appearance","External Factors","","","","","Spot derusting & painting completed. Blower casing washed with oxalic acid. Pics updated in weekly maintenance report","2020-10-06","","Completed","2020-09-11","No","No","No","Internal"]
[null,null,null,null,14015,"48_15/09/2020 11:35:51 AM","2020-09-06","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","HHC manhole door and area below grating to clean / paint.","Miscellaneous","General Appearance","External Factors","","","","","Derusting & painting of HHC manhole 4nos completed. ","2020-09-16","","Completed","2020-09-15","No","No","No","Internal"]
[null,null,null,null,14016,"48_15/09/2020 11:19:56 AM","2020-09-06","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Ladder of masthead at midship rusted.  Maintenance to be carried out","Deck - Pipe / Fittings","General Appearance","External Factors","11.1","High","","","Derusting & painting of ladder completed","2020-09-16","","Completed","2020-09-15","No","No","No","Internal"]
[null,null,null,null,14017,"48_15/9/2020 2:31:38 PM","2020-09-06","Observation","Owner / Marine / Tech. Suptd.","Engineering Audit","BWTS Line near the expansion tank covered with salt, it appears while operation it leaks. TO rectify ","E/R - Pipes/ valves & fittings","General Appearance","Equipment Related","","","","","BWTS Line near the expansion leaks rectified. ","2020-09-16","","Completed","2020-09-13","No","No","No","Internal"]
[null,null,null,null,14018,"48_15/9/2020 2:41:13 PM","2020-09-06","Observation","Owner / Marine / Tech. Suptd.","Engineering Audit","DG Exhaust pipe seal pot not having water. To top up water and maintain","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","DG Exhaust pipe seal pot topped up with water.","2020-09-13","","Completed","2020-09-09","No","No","No","Internal"]
[null,null,null,null,14019,"48_15/09/2020 11:15:36 AM","2020-09-06","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Gas alarm for A deck entrance door found active in CCR. ","Miscellaneous","Safety / LSA / FFA","Equipment Related","","","","","Calibration of accommodation fixed gas detection system to be carried out using SPAN gas ","2020-09-12","","Completed","2020-09-12","No","No","No","Internal"]
[null,null,null,null,14020,"48_15/09/2020 11:32:38 AM","2020-09-06","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Water found accumulated in both life boat. To clean dry and to check source of water leak","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.29","High","","","Upon investigation it was found that the gasket for forward pothole on P-side lifeboat & Aft porthole for S-Lifeboat (rubber packing damaged) was leaking slightly ,also it was found that  butterfly nuts securing frame  on window was bent. Repairs carried out on butterfly securing arrangement & tested. No leak observed after repairs","2020-09-16","STAI200217","Completed","2020-09-16","No","No","No","Internal"]
[null,null,null,null,14021,"48_15/9/2020 2:27:42 PM","2020-09-06","Other","Owner / Marine / Tech. Suptd.","Engineering Audit","Aux boiler uptake cladding has dislodged","E/R - Pipes/ valves & fittings","General Appearance","Equipment Related","","","","","Aux boiler uptake cladding riveted and repaired","2020-09-21","","Completed","2020-09-16","No","No","No","Internal"]
[null,null,null,null,14022,"48_15/9/2020 2:38:23 PM","2020-09-06","Observation","Owner / Marine / Tech. Suptd.","Engineering Audit","Aux boiler no 1 main steam stop valve has steam leak, to remove the lagging, locate the leak and rectify","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","Valve Bonnet opened. Changed the gasket","2020-10-06","","Completed","2020-09-18","No","No","No","Internal"]
[null,null,null,null,null,"48_15/09/2020 11:44:51 AM","2020-09-06","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Engine casing bulkhead which are in shadow of the scrubber room has all turned yellow. Maintenance required for the same.","Miscellaneous","General Appearance","External Factors",null,null,"Not Applicable","Not Applicable","Spot derusting & painting required on funnel casing. Vessel experiencing rolling upto 8deg in Indian ocean. Work aloft to be undertaked when favourable conditions are achived","2020-10-06",null,"Completed","2020-10-08","No",null,null,"Internal"]
[null,null,null,null,null,"48_17/09/2020 1:37:08 PM","2020-09-06","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","All winches and windlasses gear oil to be checked as some appeared emulsified and above sight glass level.","Deck - Mooring Machinery","Mooring","Equipment Related",9.14,"Medium","Not Applicable","Not Applicable","Hydraulic oil renewed for all mooring winches enclosed gears. Sight glass cleaned from inside. Oil level visible clearly in all mooring winches.\r\n","2020-11-30",null,"Completed","2020-11-22","No",null,null,"Internal"]
[null,null,null,null,14023,"48_16/9/2020 8:57:40 AM","2020-09-10","Defect","Ship Staff","Ship Staff Insp.","No:1 LT cooler sea water inlet line sacrificial flange leak.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","No.1 LT cooler sea water inlet line sacrificial  flange renewedwith new spare. All gasket laso replaced with new one.","2020-11-10","","Completed","2020-09-17","No","No","No","Internal"]
[null,null,null,null,14024,"48_16/9/2020 8:59:15 AM","2020-09-10","Defect","Ship Staff","Ship Staff Insp.","No:2 LT cooler sea water inlet line sacrificial  flange leak.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","No.2 LT cooler sea water inlet line sacrificial  flange renewedwith new spare. All gasket also replaced with new one.","2020-11-10","","Completed","2020-09-17","No","No","No","Internal"]
[null,null,null,null,null,"48_17/9/2020 4:12:42 PM","2020-09-14","Defect","Ship Staff","Ship Staff Insp.","THE lUBRICATOR VENT IS KEPT OPENED FOR NO. 1 UNIT. IT IS LEAKING THERE ALL THE TIME.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related",null,null,"Not Applicable","Not Applicable","ME Lubricator oil leak checked for leakage, all flanged for double wall pipe slacked and found Cylinder lubricator No.5 unit checked and fittings leakaged on the copper gasket. Same replaced with new spare gasket. Servo oil Inlet pipe on no.7 unit copper gasket also same replaced with new one. ","2020-12-14",null,"Completed","2020-10-27","No",null,null,"Internal"]
[null,null,null,null,null,"48_17/9/2020 6:46:54 PM","2020-09-17","Defect","Ship Staff","Ship Staff Insp.","Drinking water Tank outlet valve found not holding.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related",null,null,"Not Applicable","Not Applicable","Drinking water tank made empty. Changed the valve with new","2020-11-17",null,"Completed","2020-11-07","No",null,null,"Internal"]
[null,null,null,null,14170,"48_03/10/2020 4:02:14 PM","2020-09-19","Defect","Ship Staff","Suptd. Insp.","Operating lever for P/room davit faulty. The lever is not resting in neutral position fute faulty mechanish.","Deck - Machinery","ISM Related","Equipment Related","","","","","Operating lever for P/room davit inspected. maintenance carried out. P/room davit operation tested after maintenance, found in good working condition","2020-09-30","","Completed","2020-09-27","No","No","No","Internal"]
[null,null,null,null,14012,"48_19/09/2020 11:19:45","2020-09-19","Defect","Ship Staff","Ship Staff Insp.","The GMT timing in the EGCS panel is 10 mins behind the actual GMT timing.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Changed the GMT timings as per the advise from the maker ","2020-11-19","","Completed","2020-09-25","No","No","No","Internal"]
[null,null,null,null,null,"48_23/9/2020 12:30:13 PM","2020-09-23","Defect","Ship Staff","Ship Staff Insp.","ME fuel pump no 4 high temprature sensor diffective.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related",null,null,"Not Applicable","Not Applicable","Sensor replaced with new sapre ","2020-12-23","STAI200220","Completed","2020-10-24","No",null,null,"Internal"]
[null,null,null,null,null,"48_26/9/2020 12:19:26 PM","2020-09-26","Defect","Ship Staff","Ship Staff Insp.","Aux CSW pump no.1 suction valve suspected not holding ","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related",null,null,"Not Applicable","Not Applicable","Aux CSW pump no.1 suction vlave checked found in good condition same cleaned. Discharge valve found seat have deep cut same replaced with new spare.","2020-12-26","STAI200221","Completed","2020-10-29","No",null,null,"Internal"]
[null,null,null,null,null,"48_03/10/2020 3:57:59 PM","2020-09-30","Defect","Ship Staff","Ship Staff Insp.","Accommodation fixed gas detection system System Fault alarm is triggered on bridge & E/R. Display is blank & not responding. ","Accommodation","Safety / LSA / FFA","Equipment Related",null,null,"Not Applicable","Not Applicable","Display unit replaced with spare new.","2020-11-30",null,"Completed","2020-11-14","No",null,null,"Internal"]
[null,null,null,null,null,"48_31/10/2020 8:50:57 AM","2020-10-19","Critical Equipment","Ship Staff","Ship Staff Insp.","Forward whistle found inoperative after vessel experienced bad weather in south china sea. ","Navigation - Others","Navigation","Equipment Related",null,null,"Not Applicable","Not Applicable","Forward whistle motor overhauled, bearings & crankshft renewed with spare available onboard. After installation operation tested of the whistle, found in good working condition","2020-12-18",null,"Completed","2020-10-28","No",null,null,"Internal"]
[null,null,null,null,null,"48_31/10/2020 8:40:52 AM","2020-10-23","Observation","Ship Staff","Ship Staff Insp.","Oil dripping from STBD windlass operating lever control assembly.","Deck - Machinery","Mooring","Equipment Related",9.14,"Medium","Not Applicable","Not Applicable","O-Ring for windlass operating lever renewed & tested. no leaks observed after replacement. Spare O-rings & plugs needs to be ordered for future troubleshooting","2020-10-30",null,"Completed","2020-10-26","No",null,null,"Internal"]
[null,null,null,null,null,"48_31/10/2020 8:44:17 AM","2020-10-24","Observation","Ship Staff","Ship Staff Insp.","Spring line mooring winch M4 hydraulic oil return line found leaking. It was noted that the pipe was repaired in the past & needs replacement","Deck - Mooring Machinery","Mooring","Equipment Related",9.14,"Medium","Not Applicable","Not Applicable","Section of thye return line for hydraulic line replaced with new pipe fabricated onboard.","2020-10-31",null,"Completed","2020-10-31","No",null,null,"Internal"]
[null,null,null,null,null,"48_01/12/2020 10:26:52 PM","2020-11-05","Defect","Ship Staff","Ship Staff Insp.","4 nos COW machines (2nos from 1C & 2nos from 2C COT ) found inoperative or working intermittently during discharging operation at Daxie oil terminal. ","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related",null,null,"Not Applicable","Not Applicable","4nos of COW machines overhauled (gun unit & driving unit) after removing from the tank. Machies manually tested for smooth movement after overhauling, found in good working condition. ","2021-01-04",null,"Completed","2020-12-07","No",null,null,"Internal"]
[null,null,null,null,null,"48_30/11/2020 14:33:25","2020-11-28","Defect","Ship Staff","Ship Staff Insp.","SENSOR FOR T/C RPM FOR AUX ENGINE NOT OPERATIONAL","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related",null,null,"Not Applicable","Not Applicable","Removed T/C and fitted the sensor back. Working good","2021-06-01",null,"Completed","2020-12-02","No",null,null,"Internal"]
[null,null,null,null,null,"48_18/12/2020 11:00:51 PM","2020-12-10","Defect","Ship Staff","Ship Staff Insp.","Accommodation fixed gas detection system - Galley air intake sensor faulty (Sensor path blocked)","Accommodation","Safety / LSA / FFA","Equipment Related",null,null,"Not Applicable","Not Applicable","Sensor inspected & cleaned. Path cleared & tested. System in good working condition & no alarm in the system","2021-02-10",null,"Completed","2020-12-16","No",null,null,"Internal"]
[null,null,null,null,null,"48_15/12/2020 18:19:46","2020-12-14","Defect","Ship Staff","Ship Staff Insp.","EMERGENCY GENERATOR SPRING START STARTER NOT OPERATIONAL.","Critical Equip.","Emgcy. Systems","Equipment Related",10.34,"High","Not Applicable","Not Applicable","Overhauled the starter. Found one pin broken. same fabricated and tried out.","2020-12-28","STAI200276","Completed","2020-12-16","No",null,null,"Internal"]

{"sheet":"Calc","index":2,"n_rows":28,"n_cols":12,"rows_kept":28,"cut":false,"hidden":true,"merged":[]}
["Def_type","Def_cause","Equipments","VIQrefno","Observer_code"]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,"Dim itemSele As Long"]
[null,null,null,null,null,null,null,null,null,null,null,"   dim startRow as integer"]
[null,null,null,null,null,null,null,null,null,null,null,"   startRow=1"]
[null,null,null,null,null,null,null,null,null,null,null,"        For itemSele = 0 To ListBox1.ListCount - 1"]
[null,null,null,null,null,null,null,null,null,null,null,"        If ListBox1.Selected(itemSele) = True Then"]
[null,null,null,null,null,null,null,null,null,null,null,"        Worksheets(\"WorksheetName\").Range(\"A\" & startRow).Value = ListBox1.List(itemSele)"]
[null,null,null,null,null,null,null,null,null,null,null,"        startRow = startRow + 1"]
[null,null,null,null,null,null,null,null,null,null,null,"        End If"]
[null,null,null,null,null,null,null,null,null,null,null,"        Next"]
[null,null,null,null,null,null,null,null,null,null,null,"Dim LastRowA As String"]
[null,null,null,null,null,null,null,null,null,null,null,"        Dim itemSele As Long"]
[null,null,null,null,null,null,null,null,null,null,null,"       Dim startRow as integer"]
[null,null,null,null,null,null,null,null,null,null,null,"        LastRowA = ActiveSheet.Cells(Rows.count, \"A\").End(xlUp).row"]
[null,null,null,null,null,null,null,null,null,null,null,"        startQue = 0"]
[null,null,null,null,null,null,null,null,null,null,null,"        For itemSele = 0 To ListBox1.ListCount - 1"]
[null,null,null,null,null,null,null,null,null,null,null,"        For startRow = 1 To LastRowA"]
[null,null,null,null,null,null,null,null,null,null,null,"        If Worksheets(\"WorksheetName\").Range(\"A\" & startRow).Value = ListBox1.List(itemSele) Then"]
[null,null,null,null,null,null,null,null,null,null,null,"        ListBox1.Selected(itemSele) = True"]
[null,null,null,null,null,null,null,null,null,null,null,"        Exit For"]
[null,null,null,null,null,null,null,null,null,null,null,"        End If"]
[null,null,null,null,null,null,null,null,null,null,null,"        Next j"]
[null,null,null,null,null,null,null,null,null,null,null,"        Next"]
[null,null,null,null,null,null,null,null,null,null,null,"        End If"]

{"sheet":"Areaofobs","index":3,"n_rows":17,"n_cols":2,"rows_kept":17,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Cargo / Ballast Systems",11]
["Cert. & Docu.",2]
["Communication",6]
["Crew Management",3]
["Emgcy. Systems",13]
["Eng. / Strg. Comp.",14]
["General Appearance",15]
["Ice Opns.",17]
["ISM Related",7]
["ISPS Related",10]
["MARPOL Related",9]
["MLC Related",4]
["Mooring",12]
["Navigation",5]
["Safety / LSA / FFA",8]
["Structural Condn. / WT integrity ",16]

{"sheet":"Vessel_type","index":4,"n_rows":1,"n_cols":2,"rows_kept":1,"cut":false,"hidden":true,"merged":[]}
["Vessel_type","ID"]

{"sheet":"Deficiency_type","index":5,"n_rows":8,"n_cols":3,"rows_kept":8,"cut":false,"hidden":true,"merged":[]}
["TITLE","Type of deficiency_description","ID"]
["Breakdown",null,6]
["Critical Equipment",null,4]
["Defect",null,1]
["Guarantee Claim",null,8]
["Non Conformity",null,2]
["Observation",null,3]
["Other",null,7]

{"sheet":"VIQrefno","index":6,"n_rows":427,"n_cols":3,"rows_kept":427,"cut":false,"hidden":true,"merged":[]}
["VIQ_ref_no","Risk Value of observation","ID"]
["1.1","Low",8243]
["1.10","Low",8252]
["1.11","Low",8253]
["1.12","Low",8254]
["1.13","Low",8255]
["1.14","Low",8256]
["1.15","Low",8257]
["1.16","Low",8259]
["1.17","Low",8260]
["1.18","Low",8261]
["1.19","Low",8262]
["1.2","Low",8244]
["1.20","Low",8263]
["1.21","Low",8265]
["1.22","Low",8266]
["1.23","Low",8267]
["1.24","Low",8268]
["1.25","Low",8269]
["1.26","Low",8270]
["1.3","Low",8245]
["1.4","Low",8246]
["1.5","Low",8247]
["1.6","Low",8248]
["1.7","Low",8249]
["1.8","Low",8250]
["1.9","Low",8251]
["1.99","High",11258]
["10.1","Medium",8461]
["10.10","High",8470]
["10.11","Medium",8471]
["10.12","Very High",8472]
["10.13","Very High",8473]
["10.14","Medium",8474]
["10.15","Low",8475]
["10.16","Very High",8476]
["10.17","Very High",8477]
["10.18","High",8478]
["10.19","Very High",8479]
["10.2","Low",8462]
["10.20","High",8480]
["10.21","Medium",8481]
["10.22","Low",8482]
["10.23","Medium",8483]
["10.24","Low",8484]
["10.25","Very High",8485]
["10.26","High",8486]
["10.27","Medium",8487]
["10.28","Low",8488]
["10.29","Medium",8489]
["10.3","Medium",8463]
["10.30","High",8490]
["10.31","Very High",8491]
["10.32","Very High",8492]
["10.33","High",8493]
["10.34","High",8494]
["10.35","Very High",8495]
["10.36","Very High",8496]
["10.37","Medium",8497]
["10.38","Medium",8498]
["10.39","High",8499]
["10.4","High",8464]
["10.40","Medium",8500]
["10.41","Medium",8501]
["10.42","Medium",8502]
["10.43","Medium",8503]
["10.44","Medium",8504]
["10.45","Very High",8505]
["10.46","High",8506]
["10.47","Medium",8507]
["10.48","High",8508]
["10.49","Medium",8509]
["10.5","Low",8465]
["10.50","High",8510]
["10.51","Low",8511]
["10.52","Medium",8512]
["10.53","Medium",8513]
["10.54","High",8514]
["10.55","Low",8515]
["10.6","Very High",8466]
["10.7","Medium",8467]
["10.8","Medium",8468]
["10.9","Medium",8469]
["10.99","High",8516]
["11.1","High",8420]
["11.10","Medium",8429]
["11.11","Very High",8430]
["11.12","Low",8431]
["11.13","Low",8432]
["11.14","Medium",8433]
["11.15","Low",8434]
["11.16","Low",8435]
["11.17","Low",8436]
["11.2","Medium",8421]
["11.3","Medium",8422]
["11.4","Very High",8423]
["11.5","Medium",8424]
["11.6","Medium",8425]
["11.7","High",8426]
["11.8","Low",8427]
["11.9","Low",8428]
["11.99","High",8437]
["12.1","High",8438]
["12.10","High",8448]
["12.11","High",8449]
["12.12","High",8450]
["12.13","High",8451]
["12.14","High",8452]
["12.15","High",8453]
["12.16","High",8454]
["12.17","High",8455]
["12.18","High",8456]
["12.19","High",8457]
["12.2","High",8439]
["12.20","High",8458]
["12.21","High",8459]
["12.3","High",8441]
["12.4","High",8442]
["12.5","High",8443]
["12.6","High",8444]
["12.7","High",8445]
["12.8","High",8446]
["12.9","High",8447]
["12.99","High",8460]
["2.1","Very High",8296]
["2.1.9","Very High",11259]
["2.10","Medium",8304]
["2.11","Medium",8305]
["2.12","Low",8306]
["2.13","Low",8307]
["2.14","Low",8308]
["2.15","Low",8309]
["2.16","Medium",8310]
["2.2","Medium",8297]
["2.3","High",8295]
["2.4","Medium",8298]
["2.5","Medium",8299]
["2.6","Low",8300]
["2.7","High",8301]
["2.8","High",8302]
["2.9","Medium",8303]
["2.99","High",8311]
["3.1","High",8312]
["3.2","Very High",8313]
["3.3","High",8314]
["3.4","Low",8294]
["3.5","Medium",8315]
["3.6","High",8316]
["3.7","Very High",8317]
["3.8","Very High",8318]
["3.99","High",8319]
["4.1","High",8320]
["4.10","High",8329]
["4.11","Medium",8330]
["4.12","Very High",8331]
["4.13","Very High",8332]
["4.14","Very High",8333]
["4.15","Very High",8334]
["4.16","Very High",8335]
["4.17","Very High",8336]
["4.18","Very High",8337]
["4.19","Low",8338]
["4.2","Medium",8321]
["4.20","Very High",8339]
["4.21","High",8340]
["4.22","Low",8341]
["4.23","High",8342]
["4.24","High",8343]
["4.25","Low",8344]
["4.26","Low",8345]
["4.27","High",8346]
["4.3","Medium",8322]
["4.4","High",8323]
["4.5","Very High",8324]
["4.6","Medium",8325]
["4.7","High",8326]
["4.8","Medium",8327]
["4.9","Medium",8328]
["4.99","High",8347]
["5.1","Very High",8517]
["5.10","High",8526]
["5.11","Low",8527]
["5.12","Medium",8528]
["5.13","High",8529]
["5.14","Very High",8530]
["5.15","Medium",8531]
["5.16","Very High",8532]
["5.17","Very High",8533]
["5.18","High",8534]
["5.19","Medium",8535]
["5.2","Very High",8518]
["5.20","Medium",8536]
["5.21","Medium",8537]
["5.22","High",8539]
["5.23","Very High",8540]
["5.24","Very High",8541]
["5.25","Medium",8542]
["5.26","Medium",8543]
["5.27","Medium",8544]
["5.28","Very High",8545]
["5.29","High",8546]
["5.3","Low",8519]
["5.30","High",8547]
["5.31","High",8548]
["5.32","High",8549]
["5.33","High",8550]
["5.34","Low",8551]
["5.35","Medium",8552]
["5.36","Low",8553]
["5.37","Low",8554]
["5.38","High",8555]
["5.39","Very High",8556]
["5.4","High",8520]
["5.40","Very High",8557]
["5.41","Very High",8558]
["5.42","Medium",8559]
["5.43","High",8560]
["5.44","High",8561]
["5.45","Medium",8564]
["5.46","Medium",8565]
["5.47","Medium",8566]
["5.48","Medium",8567]
["5.5","Low",8521]
["5.6","Low",8522]
["5.7","Medium",8523]
["5.8","Medium",8524]
["5.9","Very High",8525]
["5.99","High",8568]
["6.1","Medium",8348]
["6.10","Low",8357]
["6.11","High",8358]
["6.12","Medium",8359]
["6.13","Low",8360]
["6.14","High",8361]
["6.15","High",8362]
["6.16","Very High",8363]
["6.17","Very High",8364]
["6.18","Medium",8365]
["6.19","Low",8366]
["6.2","High",8349]
["6.20","Medium",8367]
["6.21","High",8368]
["6.22","Medium",8369]
["6.3","Low",8350]
["6.4","High",8351]
["6.5","Medium",8352]
["6.6","Medium",8353]
["6.7","High",8354]
["6.8","High",8355]
["6.9","Low",8356]
["6.99","High",8370]
["7.1","High",8371]
["7.10","High",8380]
["7.11","High",8381]
["7.12","High",8382]
["7.13","Medium",8383]
["7.14","Medium",8384]
["7.15","High",8385]
["7.16","High",8386]
["7.17","High",8387]
["7.2","High",8372]
["7.3","Low",8373]
["7.4","Low",8374]
["7.5","Low",8375]
["7.6","Medium",8376]
["7.7","Low",8377]
["7.8","High",8378]
["7.9","High",8379]
["7.99","High",8388]
["8.1","Very High",8569]
["8.10","Very High",8578]
["8.100","Low",11227]
["8.101","Medium",11228]
["8.102","Low",11229]
["8.103","Low",11230]
["8.104","Low",11231]
["8.105","Medium",11232]
["8.106","Medium",11233]
["8.107","Low",11234]
["8.108","High",11235]
["8.109","Very High",11236]
["8.11","Medium",8579]
["8.110","High",11237]
["8.111","Medium",11238]
["8.112","High",11239]
["8.113","Medium",11240]
["8.114","Low",11241]
["8.115","High",11242]
["8.116","Medium",11243]
["8.117","Medium",11244]
["8.118","Medium",11245]
["8.119","High",11246]
["8.12","Medium",8580]
["8.120","High",11247]
["8.121","Medium",11248]
["8.122","High",11249]
["8.123","High",11250]
["8.124","Low",11251]
["8.125","High",11252]
["8.126","Medium",11253]
["8.127","Medium",11254]
["8.13","Medium",8581]
["8.14","Very High",8582]
["8.15","High",8583]
["8.16","Very High",8584]
["8.17","Low",8585]
["8.18","High",8586]
["8.19","High",8587]
["8.199","High",11255]
["8.2","Medium",8570]
["8.20","Medium",8588]
["8.21","High",8589]
["8.22","Very High",8590]
["8.23","Medium",8591]
["8.24","Medium",8592]
["8.25","Very High",8593]
["8.26","High",8594]
["8.27","Medium",8595]
["8.28","Medium",8596]
["8.29","High",8598]
["8.3","Very High",8571]
["8.30","High",8599]
["8.31","High",8600]
["8.32","Low",8601]
["8.33","Medium",8602]
["8.34","High",8603]
["8.35","Medium",8604]
["8.36","Medium",8605]
["8.37","High",8607]
["8.38","Medium",8608]
["8.39","Medium",8609]
["8.4","Medium",8572]
["8.40","High",8610]
["8.41","Medium",8611]
["8.42","Medium",8612]
["8.43","Very High",8613]
["8.44","High",8615]
["8.45","High",8616]
["8.46","Very High",8617]
["8.47","Very High",8618]
["8.48","Medium",8619]
["8.49","High",8620]
["8.5","Very High",8573]
["8.50","Medium",8621]
["8.51","Low",8622]
["8.52","Low",8623]
["8.53","Low",8624]
["8.54","High",8625]
["8.55","Low",11182]
["8.56","Medium",11183]
["8.57","Medium",11184]
["8.58","High",11185]
["8.59","High",11186]
["8.6","Medium",8574]
["8.60","High",11187]
["8.61","Medium",11188]
["8.62","Very High",11189]
["8.63","High",11190]
["8.64","Medium",11191]
["8.65","Low",11192]
["8.66","High",11193]
["8.67","High",11194]
["8.68","High",11195]
["8.69","Medium",11196]
["8.7","High",8575]
["8.70","Medium",11197]
["8.71","Very High",11198]
["8.72","Medium",11199]
["8.73","Medium",11200]
["8.74","High",11201]
["8.75","Medium",11202]
["8.76","Medium",11203]
["8.77","Medium",11204]
["8.78","Medium",11205]
["8.79","Medium",11206]
["8.8","Medium",8576]
["8.80","Medium",11207]
["8.81","Low",11208]
["8.82","Medium",11209]
["8.83","Low",11210]
["8.84","Low",11211]
["8.85","Medium",11212]
["8.86","Medium",11213]
["8.87","Medium",11214]
["8.88","Low",11215]
["8.89","High",11216]
["8.9","High",8577]
["8.90","High",11217]
["8.91","High",11218]
["8.92","Medium",11219]
["8.93","Low",11220]
["8.94","Low",11221]
["8.95","Medium",11222]
["8.96","Medium",11223]
["8.97","Low",11224]
["8.98","High",11225]
["8.99","Medium",11226]
["9.1","Low",8390]
["9.10","Medium",8399]
["9.11","Medium",8400]
["9.12","Medium",8401]
["9.13","Low",8402]
["9.14","Medium",8403]
["9.15","Medium",8404]
["9.16","High",8405]
["9.17","High",8406]
["9.18","Low",8407]
["9.19","Low",8408]
["9.2","Very High",8391]
["9.20","Medium",8409]
["9.21","Medium",8410]
["9.22","Low",8411]
["9.23","Low",8412]
["9.24","Medium",8413]
["9.25","Low",8414]
["9.26","Low",8415]
["9.27","Low",8416]
["9.28","Medium",8417]
["9.29","Low",8418]
["9.3","Very High",8392]
["9.4","High",8393]
["9.5","High",8394]
["9.6","Low",8395]
["9.7","Medium",8396]
["9.8","Medium",8397]
["9.9","Medium",8398]
["9.99","High",8419]

{"sheet":"Equipment_list","index":7,"n_rows":28,"n_cols":3,"rows_kept":28,"cut":false,"hidden":true,"merged":[]}
["TITLE","Equipment_list_description","ID"]
["Accommodation",null,12]
["Cargo Mach.",null,13]
["Critical Equip.",null,16]
["Deck - Machinery",null,18]
["Deck - Mooring Machinery",null,15]
["Deck - Pipe / Fittings",null,20]
["Documentation",null,21]
["E/R - Air Comp.",null,8]
["E/R - Aux. Engine",null,4]
["E/R - Aux. Mach.",null,7]
["E/R - Boiler",null,5]
["E/R - Main Engine",null,3]
["E/R - Pipes/ valves & fittings",null,9]
["E/R - Pumps",null,32]
["E/R - Purifier",null,6]
["Elect. Mach. & Equip.",null,10]
["Hull & Tanks",null,19]
["Inert Gas",null,14]
["LSA / FFA",null,17]
["Miscellaneous",null,22]
["Navigation - DGPS / EPFS / AIS",null,28]
["Navigation - ECDIS",null,25]
["Navigation - Echo Sounder / Speed Log",null,26]
["Navigation - GMDSS & Communication",null,23]
["Navigation - Others",null,11]
["Navigation - RADAR",null,24]
["Navigation - VDR / BNWAS",null,30]

{"sheet":"PSC_MOU","index":8,"n_rows":11,"n_cols":3,"rows_kept":11,"cut":false,"hidden":true,"merged":[]}
["TITLE","PSC_MOU_description","ID"]
["Asia and the Pacific",null,2]
["Caribbean",null,4]
["Europe and the North Atlantic",null,1]
["Latin America",null,3]
["The Black Sea region",null,6]
["The Indian Ocean",null,8]
["The Mediterranean",null,7]
["The Riyadh MoU",null,9]
["USCG",null,10]
["West and Central Africa",null,5]

{"sheet":"Inspection_type","index":9,"n_rows":13,"n_cols":2,"rows_kept":13,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Bunkering Audit",14]
["Cargo Audit",17]
["Engineering Audit",16]
["ISM Audit",2]
["ISPS Audit",3]
["IT Audit",10]
["MLC Audit",1]
["Mooring Audit",9]
["Nav Audit / Verification",8]
["Onboard Training",18]
["Ship Staff Insp.",15]
["Suptd. Insp.",13]

{"sheet":"Deficiency_Cause","index":10,"n_rows":8,"n_cols":3,"rows_kept":8,"cut":false,"hidden":true,"merged":[]}
["TITLE","Deficiency_Cause_description","ID"]
["Behaviour Based",null,1]
["Equipment Related",null,4]
["External Factors",null,5]
["Human Error",null,7]
["Inappropriate Procedure",null,8]
["Industry Issue",null,6]
["Knowledge Based",null,3]

{"sheet":"Observer_code","index":11,"n_rows":3,"n_cols":3,"rows_kept":3,"cut":false,"hidden":true,"merged":[]}
["TITLE","Observer_code_description","ID"]
["Owner / Marine / Tech. Suptd.",null,3]
["Ship Staff",null,2]

{"sheet":"Status_code","index":12,"n_rows":8,"n_cols":3,"rows_kept":8,"cut":false,"hidden":true,"merged":[]}
["TITLE","Status_code_description","ID"]
[]
["Completed",null,6]
["Deferred to D D",null,5]
["In progress",null,3]
["Not Started",null,2]
["Waiting spare",null,4]
["xyz",null,8]

{"sheet":"PSC_ref_no","index":13,"n_rows":19,"n_cols":2,"rows_kept":19,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Alarms",9]
["Cargo operations including equipment",7]
["Certificates & Documentation",2]
["Dangerous Goods",13]
["Emergency Systems",5]
["Fire safety",8]
["ISM",16]
["ISPS",17]
["Life saving appliances",12]
["MLC, 2006",18]
["Other",19]
["Pollution Prevention",15]
["Propulsion and auxiliary machinery",14]
["Radio communication",6]
["Safety of Navigation",11]
["Structural condition",3]
["Water/Weathertight condition",4]
["Working and Living Conditions",10]

{"sheet":"Risk_value_of_obs","index":14,"n_rows":1,"n_cols":2,"rows_kept":1,"cut":false,"hidden":true,"merged":[]}
["Risk Value of observation","ID"]

{"sheet":"Year","index":15,"n_rows":18,"n_cols":1,"rows_kept":18,"cut":false,"hidden":true,"merged":[]}
["Year"]
[2014]
[2015]
[2016]
[2017]
[2018]
[2019]
[2020]
[2021]
[2022]
[2023]
[2024]
[2025]
[2026]
[2027]
[2028]
[2029]
[2030]

{"sheet":"Month","index":16,"n_rows":13,"n_cols":1,"rows_kept":13,"cut":false,"hidden":true,"merged":[]}
["Month"]
["Jan"]
["Feb"]
["Mar"]
["Apr"]
["May"]
["Jun"]
["Jul"]
["Aug"]
["Sep"]
["Oct"]
["Nov"]
["Dec"]

{"sheet":"Date_","index":17,"n_rows":32,"n_cols":1,"rows_kept":32,"cut":false,"hidden":true,"merged":[]}
["Date"]
["01"]
["02"]
["03"]
["04"]
["05"]
["06"]
["07"]
["08"]
["09"]
[10]
[11]
[12]
[13]
[14]
[15]
[16]
[17]
[18]
[19]
[20]
[21]
[22]
[23]
[24]
[25]
[26]
[27]
[28]
[29]
[30]
[31]

{"sheet":"Sheet1","index":18,"n_rows":24,"n_cols":6,"rows_kept":24,"cut":false,"hidden":true,"merged":[]}
[]
[null,"ID","E",null,"Date Recorded",1]
[null,"UNIQUE ID","F",null,"Type of Deficiency",2]
[1,"Date Recorded","G",null,"Observer code",3]
["ignore","Vessel Type","H",null,"Type of Inspection",4]
[null,"Internal / External","I",null,"Description of Deficiency",5]
[null,"Drydock","J",null,"Equipment Categories",6]
[null,"Information Sharing","K",null,"Area of Observation",7]
[null,"Critical_item","L",null,"Deficiency Cause",8]
[null,"Deficiency Type","M",null,"VIQ Ref Number",9]
[null,"Deficiency Cause","N",null,"Risk Value of Obs",10]
[null,"Inspection Type","O",null,"PSC Ref Number",11]
[null,"Equipments","P",null,"PSC MOU ID",12]
[null,"VIQ Reference Number","Q",null,"Action Taken or Required",13]
[null,"Risk Value of the observation","R",null,"Target Date",14]
[null,"PSC Reference Number","S",null,"PO Ref No.",15]
[null,"PSC MOU","T",null,"Status Code",16]
[null,"Observer Code","U",null,"Date Completed",17]
[null,"Target Date","V",null,"Drydock",18]
[null,"Status Code","W",null,"Info Sharing",19]
[null,"Description of Deficiency","X",null,"Critical Item Flag",20]
[null,"Action taken / required","Y",null,"Audit Type",21]
[null,"PO ref no","Z"]
[null,"Date completed","AA"]

{"sheet":"Ship_information","index":19,"n_rows":2,"n_cols":3,"rows_kept":2,"cut":false,"hidden":true,"merged":[]}
["Ship_ID","Ship_Name","FILE_NAME"]
["48","DHT TAIGA (19-09-2020)","48_1602039563413.xlsm"]

{"sheet":"External_Deficiency_type","index":20,"n_rows":5,"n_cols":3,"rows_kept":5,"cut":false,"hidden":true,"merged":[]}
["TITLE","Type of deficiency_description","ID"]
["Condn of Class / Memo",null,5]
["Defect",null,1]
["Non Conformity",null,2]
["Observation",null,3]

{"sheet":"External_Inspection_type","index":21,"n_rows":11,"n_cols":2,"rows_kept":11,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Cargo Audit",17]
["Flag State Insp.",5]
["ISM Audit",2]
["ISPS Audit",3]
["MLC Audit",1]
["Nav Audit / Verification",8]
["OM Insp. (Eg. SIRE / CDI etc.)",6]
["Others (Eg. Insurance etc.)",12]
["PSC Inspection",4]
["Terminal Insp.",11]

{"sheet":"External_Observer_code","index":22,"n_rows":7,"n_cols":3,"rows_kept":7,"cut":false,"hidden":true,"merged":[]}
["TITLE","Observer_code_description","ID"]
["Class Surveyor",null,4]
["FSC Inspector",null,5]
["Others (Eg. Insurance etc.)",null,9]
["PSC Insp.",null,6]
["SIRE / CDI Insp.",null,8]
["Terminal Insp.",null,7]

{"sheet":"Sheet Version","index":23,"n_rows":2,"n_cols":2,"rows_kept":2,"cut":false,"hidden":true,"merged":[]}
["Version","Title"]
["2.0","Version 2.0"]