{"text_format":"1","workbook":"xlsx","n_sheets":24,"sheets":["Mainsheet","Completed","Calc","Areaofobs","Vessel_type","Deficiency_type","VIQrefno","Equipment_list","PSC_MOU","Inspection_type","Deficiency_Cause","Observer_code","Status_code","PSC_ref_no","Risk_value_of_obs","Year","Month","Date_","Sheet1","Ship_information","External_Deficiency_type","External_Inspection_type","External_Observer_code","Sheet Version"],"not_rendered":{"charts":0,"images":5,"macros":1,"external_links":0,"defined_names":12,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Mainsheet","index":0,"n_rows":48,"n_cols":28,"rows_kept":48,"cut":false,"hidden":false,"merged":[[10,8,10,9],[10,12,10,13],[12,6,12,27],[8,6,8,27]]}
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,"Defect - Damage Monitoring Sheet"]
[]
[null,null,null,null,null,null,null,"Date of Report","01-Dec-2020",null,null,"Ship Name","EAGLE (12-06-2020)"]
[]
[null,null,null,null,null,null,"VERSION : 2.0"]
[]
[]
[]
[null,null,null,null,"ID","UNIQUE ID","Date Recorded","Type of Deficiency","Observer code","Type of Inspection","Description of Deficiency","Equipment Categories","Area of Observation","Deficiency Cause","VIQ Ref Number","Risk Value of Obs","PSC Ref Number","PSC MOU ID","Action Taken or Required","Target Date","PO Ref No.","Status Code","Date Completed","Drydock","Info Sharing","Critical Item","Audit Type","Superintendent Remarks"]
[null,null,null,null,5164,"38_25/10/2019 6:35:06 PM","2019-05-17","Defect","Ship Staff","Ship Staff Insp.","M.E T/C No.1 tachometer not functional since DD. Sensor damaged during DD.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.11","Medium","","","Spares received. And job will be carried at anchorage.","2019-12-31","","Not Started",null,"No","No","No","Internal","plan the job at long anchorage"]
[null,null,null,null,5177,"38_2019-10-25 19:14:03.999","2019-08-28","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Accommodation front and below bridge wings area have spot rust. To be de-rusted and painted.","Accommodation","General Appearance","External Factors","11.1","High","","","PLANNED DURING CALM SEA CONDITIONS OR WHEN VESSEL AT ANCHOR. TO BE COMPLETED PROGRESSIVELY","2020-02-27","","Not Started",null,"No","No","No","Internal","Pls revert with update on progress of said job, based on percentage basis."]
[null,null,null,null,5174,"38_25/10/2019 7:06:43 PM","2019-08-30","Defect","Ship Staff","Ship Staff Insp.","Draft gauge port midship reading differs from visual more than 50 cm. Fwd and Aft gauges when loaded are indicating error of more than 50 cms","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.12","Medium","","","Planned to investigate and rectify","2020-01-31","","Not Started",null,"No","No","No","Internal","Understand that you had planned to investigate same end last month. What were your findings and recommendations to verify same?"]
[null,null,null,null,7787,"38_Mon Dec 16 2019 08:59:11 GMT+0000 (Coordinated Universal Time)","2019-12-07","Defect","Ship Staff","Ship Staff Insp.","EMBARKATION LADDER ROPES NOT IN GOOD CONDITION","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.47","Medium","","","IN PROGRESS","2020-01-20","","In progress",null,"No","No","No","Internal","its almost month, why are we not able to replace them?"]
[null,null,null,null,7792,"38_Mon Dec 16 2019 11:08:49 GMT+0000 (Coordinated Universal Time)","2019-12-15","Defect","Ship Staff","Ship Staff Insp.","Front facing port holes have become opaque, causing no clear visibilty from CCR and accomodation cabins.","Miscellaneous","General Appearance","Equipment Related","11.3","Medium","","","RO raised for new port holes. Vessel to renew port holes when rcvd.","2020-01-31","EAGL190091","In progress",null,"No","No","No","Internal","checked onboard & found glass still in acceptable limits."]
[null,null,null,null,7793,"38_Mon Dec 16 2019 11:13:16 GMT+0000 (Coordinated Universal Time)","2019-12-15","Defect","Ship Staff","Ship Staff Insp.","Crew mess room and officer's cabin carpet, ECR linolium in very bad condition. Needs renewal.","Miscellaneous","General Appearance","External Factors","11.8","Low","","","Vessel has raised RO for new carpet and Linolium. Ship staff to renew the same once rcvd.","2020-01-31","EAGL190093","In progress",null,"No","No","No","Internal","carpet cleaner & reagent provided to vessel"]
[null,null,null,null,12289,"38_18-Jan-20 2:29:59 PM","2020-01-12","Defect","Ship Staff","Ship Staff Insp.","Stbd hose handling crane, electric motor space vent wasted, crane grating securing clamps missing, angle indicator not working.","Deck - Machinery","Structural Condn. / WT integrity ","Equipment Related","8.5","Very High","","","to fabricate & renew, grating clamps to fix in place,angle indicator to be made operational.","2020-02-15","","Not Started",null,"No","No","No","Internal"]
[null,null,null,null,12282,"38_14/01/2020 1:42:16 PM","2020-01-14","Defect","Ship Staff","Ship Staff Insp.","VHF transreceiver not working from port or stbd bridge wing","Navigation - DGPS / EPFS / AIS","Navigation","Equipment Related","","","","","plug in sockets found damaged, Also Wiring from Wheel house to Bridge wing is in bad condition need to be change in Dry dock","2020-01-31","","Deferred to D D",null,"Yes","No","No","Internal","attendance carried out & rectified"]
[null,null,null,null,12355,"38_27-Jan-20 1:33:02 PM","2020-01-24","Defect","Ship Staff","Ship Staff Insp.","Port provision crane limit switch found inoperational, due to gear chain not connected to the gear. Kink observed in port side crane hoisting wire, no strands broken","Deck - Machinery","","Equipment Related","8.5","Very High","","","Investigation to be done. Chain to be put back in gear. Reqn raised for new hoisting wire. EAGL200057","2020-02-15","","Waiting spare",null,"No","No","No","Internal"]
[null,null,null,null,12363,"38_03-Mar-20 9:54:54 AM","2020-02-10","Defect","Ship Staff","Ship Staff Insp.","One of the window glass of the port side lifeboat broke during 3monthly lifeboat lowering and manoeuvering drill ","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","Temporary Acrelic sheet is fitted on the window. New glass cover is ordered. EAGL200097. Awaiting spare for permanent repairs.","2020-03-31","","Waiting spare",null,"No","No","No","Internal"]
[null,null,null,null,12364,"38_03-Mar-20 9:51:49 AM","2020-02-10","Defect","Ship Staff","Ship Staff Insp.","One of the propeller blade of POrt side lifeboat found chipped off from the edge and other found slighly bent.","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","New propeller blade to be procured and fitted. EAGL200097","2020-03-31","","Waiting spare",null,"No","No","No","Internal"]
[null,null,null,null,15317,"38_11-Jun-20 4:18:05 AM","2020-05-14","Defect","Ship Staff","Ship Staff Insp.","Slop (P) tank valve CO 537 F found to closing automatically when the valve knob put in neutral position.","Deck - Machinery","Cargo / Ballast Systems","Equipment Related","","","","","Valve block and solonoid to be inspected located in hydraulic room. Suspect leakages in valve block due to damage of O-rings.","2020-08-14","","In progress",null,"No","No","No","Internal"]
[null,null,null,null,15315,"38_17/06/2020 10:35:43 AM","2020-05-25","Defect","Ship Staff","Ship Staff Insp.","Aux Boiler No 1 and 2 emergency firing not operational","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","found FD fan potentiometer no responding when operated for the purging operation","2020-07-20","","In progress",null,"No","No","No","Internal"]
[null,null,null,null,15310,"38_11-Jun-20 4:26:49 AM","2020-06-04","Defect","Ship Staff","Ship Staff Insp.","Vessel lost about 100 liters of hydraulic oil during discharging. Upon investigation found COT 5(C) tank valve CO 531 have hydraulic leak.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","COT 5(C) tank valve CO 531 F isolated from solonoid valve block and found leakage stopped. For permanant repair Slop (S)/COT 5(C) to be washed and hydraulic line to be inspected. Cold repairs to be done for permanant repairs.","2020-09-04","","Not Started",null,"No","No","No","Internal"]
[null,null,null,null,15313,"38_11-Jun-20 4:38:15 AM","2020-06-04","Observation","Ship Staff","Ship Staff Insp.","One of the stantions of safety railing along the catwalk in way of COT 1 (S) broke from the base, which was welded on the main deck","Deck - Pipe / Fittings","General Appearance","Equipment Related","","","","","COT to be gas freed and hot work to be carried out for permanant repairs - Job deferred to DD","2020-09-04","","Deferred to D D",null,"No","No","No","Internal"]
[null,null,null,null,15311,"38_11-Jun-20 4:32:26 AM","2020-06-08","Defect","Ship Staff","Ship Staff Insp.","No.4(P), 4(S), 5(P) and 5(S) ballast tank dome butterfly nut hinges found broken (Total 10 nos.).","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","Equipment Related","","","","","New lugs to be fabricated and hot work require after offfice concurrence - Job defer to DD","2020-09-08","","Deferred to D D",null,"Yes","No","No","Internal"]
[null,null,null,null,15312,"38_11-Jun-20 4:35:12 AM","2020-06-08","Observation","Ship Staff","Ship Staff Insp.","One of the support pipe for catwalk in way of COT 3(C) found to have developed crack.","Deck - Pipe / Fittings","General Appearance","Equipment Related","","","","","Hot work require to weld the crack or sleeve to be welded after obtaining office concurrence - Job defer to DD","2020-09-08","","Deferred to D D",null,"No","No","No","Internal"]
[null,null,null,null,15337,"38_20-Nov-20 11:16:26 AM","2020-06-08","Defect","Ship Staff","Ship Staff Insp.","Many safety chain hooks along the catwalk on main deck area found broken.","Deck - Pipe / Fittings","General Appearance","Equipment Related","","","","","Temporary hook arrangment made. Defer Job to DD.","2020-09-08","","Deferred to D D",null,"No","No","No","Internal"]
[null,null,null,null,15318,"38_30/10/2020 9:32:16","2020-10-23","Defect","Ship Staff","Ship Staff Insp.","No.2 BALLAST PUMP MOTOR COUPLING TEETH FOUND DAMAGED","Cargo Mach.","Eng. / Strg. Comp.","Equipment Related","8.8","Medium","","","BALLAST PUMP COUPLING TO BE CHANGED, AS OF NOW NO SPARE AVAILABLE, REQUISITION HAS BEEN RAISED FOR SPARE COUPLING.","2020-12-23","P.O. NO. EAGL 200357","Waiting spare",null,"No","No","No","Internal"]
[null,null,null,null,15325,"38_18/11/2020 3:30:40 PM","2020-11-13","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","No.1 boiler circ. p/p oil leaking from bearing cover due to leaking seal","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","No oil seal onboard. Requisition has been raised.","2020-12-31","EAGL 200376","Waiting spare",null,"No","No","No","Internal"]
[null,null,null,null,15328,"38_18-Nov-20 6:43:30 PM","2020-11-13","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","3 ballast tank vent ordered kept in Midship locker, 2 vents to be replaced with damaged vents onboard.","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.7","High","","","2 numbers of damaged ballast tanks Vents to be replaced with new ones onboard.","2020-12-13","","Not Started",null,"No","No","No","Internal"]
[null,null,null,null,15338,"38_28/11/2020 14:34:20","2020-11-15","Defect","Ship Staff","Ship Staff Insp.","Many valve wheels on main deck corroded and wasted.","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","External Factors","","","","","To renew. RO Raised","2021-02-15","EAGL200384","Not Started",null,"No","No","No","Internal"]
[null,null,null,null,15339,"38_29/11/2020 13:34:26","2020-11-16","Critical Equipment","Ship Staff","Ship Staff Insp.","ECDIS No.2 when an alarm is generated, only visual indication of alarm is available in the display but unable to hear the Alarm Sound. ","Navigation - ECDIS","Navigation","External Factors",4.17,"Very High","Not Applicable","Not Applicable","Checked the system where the buzzer unit is connected and found It is mounted on a key board PCB, which is unable to check the status of the buzzer because of micro soldering of the PCB Board.\n\n“Generate Alarm” test carried out to confirm the same, no audible alarm is generated. - Awaiting advise form office\n\n","2020-11-30",null,"In progress",null,"No","No","No","Internal"]
[null,null,null,null,null,"38_31-Dec-20 7:47:23 PM","2020-12-07","Non Conformity","Ship Staff","Nav Audit / Verification","Handover notes of Deck Officers do not include sufficient details of status of bridge equipments.","Navigation - Others","Navigation","Human Error",null,null,"Not Applicable","Not Applicable","Deck officers were advised to write detailed status of bridge equipment in the Handover notes. ","2021-03-07",null,"In progress",null,"No",null,null,"Internal"]
[null,null,null,null,null,"38_24/12/2020 7:28:19 PM","2020-12-10","Observation","Ship Staff","Ship Staff Insp.","DGPS antenna post found rusted. ","Navigation - DGPS / EPFS / AIS","Navigation","Equipment Related",11.8,"Low","Not Applicable","Not Applicable","Temperory fixing done with cordo bond. Job reported in REFMAN for drydock.","2021-03-01",null,"Not Started",null,"Yes",null,null,"Internal"]
[null,null,null,null,null,"38_31-Dec-20 7:49:43 PM","2020-12-15","Non Conformity","Ship Staff","Nav Audit / Verification","Record of Toolbox meeting prior transiting confined water not available.","Navigation - Others","Navigation","Human Error",4.2,null,"Not Applicable","Not Applicable","Briefing carried out. Toolbox meeting and entries of the meeting to be made in Deck log/ bell book henceforth.","2021-03-15",null,"In progress",null,"No",null,null,"Internal"]
[null,null,null,null,null,"38_31-Dec-20 7:51:47 PM","2020-12-15","Non Conformity","Ship Staff","Nav Audit / Verification","Passage De-Briefing not done after completion of the voyage, same to included in company procedures","Navigation - Others","Navigation","Human Error",4.2,null,"Not Applicable","Not Applicable","After identifying, Passageplan debriefing was conducted..","2021-03-15",null,"In progress",null,"No",null,null,"Internal"]
[null,null,null,null,null,"38_31-Dec-20 7:53:55 PM","2020-12-25","Non Conformity","Ship Staff","Nav Audit / Verification","During takeover of watch, ECDIS settings not verified as per takeover checklist.","Navigation - ECDIS","Navigation","Behaviour Based",4.3,"Medium","Not Applicable","Not Applicable","ECDIS settings were verified and Checklist 12.01.35.041.02. was complied with","2021-03-25",null,"In progress",null,"No",null,null,"Internal"]
[null,null,null,null,null,"38_31-Dec-20 7:58:45 PM","2020-12-25","Non Conformity","Ship Staff","Nav Audit / Verification","Alarmable layer not plotted for No-Go areas. Marking on ENC was insufficient - Only shading done, \"No-Go Area\" was not written.","Navigation - ECDIS","Navigation","Human Error","4.15, 4.20","Very High","Not Applicable","Not Applicable","Immediately the Passage Plan was reviewed for No-Go Area marking and \"No-Go Area\" inserted in User Maps. Alarmable layers were created.","2021-03-25",null,"In progress",null,"No",null,null,"Internal"]
[null,null,null,null,null,"38_31-Dec-20 8:02:08 PM","2020-12-26","Non Conformity","Ship Staff","Nav Audit / Verification","No specific company procedures/ guidelines for carriage of minimum ENCs","Navigation - Others","Navigation","Inappropriate Procedure",null,null,"Not Applicable","Not Applicable","Office to advise and revise SMS","2021-03-26",null,"In progress",null,"No",null,null,"Internal"]
[null,null,null,null,null,"38_31-Dec-20 7:55:45 PM","2020-12-27","Non Conformity","Ship Staff","Nav Audit / Verification","BWL lowered during meal time during navigation in confined waters, without Master’s approval.","Navigation - Others","Navigation","Inappropriate Procedure",4.5999999999999996,"Medium","Not Applicable","Not Applicable","Immediately BWL was brought back to normal i.e. BWL 2.","2021-03-26",null,"In progress",null,"No",null,null,"Internal"]

{"sheet":"Completed","index":1,"n_rows":403,"n_cols":28,"rows_kept":403,"cut":false,"hidden":false,"merged":[[10,8,10,9],[10,12,10,13],[12,6,12,27],[8,6,8,27]]}
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,"Defect - Damage Monitoring Sheet"]
[]
[null,null,null,null,null,null,null,"Date of Report","01-Dec-2020",null,null,"Ship Name","EAGLE (12-06-2020)"]
[]
[null,null,null,null,null,null,"VERSION : 2.0"]
[]
[]
[]
[null,null,null,null,"ID","UNIQUE ID","Date Recorded","Type of Deficiency","Observer code","Type of Inspection","Description of Deficiency","Equipment Categories","Area of Observation","Deficiency Cause","VIQ Ref Number","Risk Value of Obs","PSC Ref Number","PSC MOU ID","Action Taken or Required","Target Date","PO Ref No.","Status Code","Date Completed","Drydock","Info Sharing","Critical Item","Audit Type","Superintendent Remarks"]
[null,null,null,null,5329,"38_26/10/2019 10:36:07 AM","2019-01-01","Defect","Ship Staff","Ship Staff Insp.","4C PV Valve found leaking","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.31","High","","","Replaced with spare O/H PV valve","2019-01-02","","Completed","2019-01-01","No","No","No","Internal"]
[null,null,null,null,5331,"38_26/10/2019 10:39:33 AM","2019-01-01","Defect","Ship Staff","Ship Staff Insp.","Electrical motor of HFO Purifier #2 Burnt, ","Elect. Mach. & Equip.","Structural Condn. / WT integrity ","Equipment Related","10.32","Very High","","","Motor Requisition received and replaced with new Motor. Purifier tried out, Performance satisfactiory","2019-01-10","","Completed","2019-01-07","No","No","No","Internal"]
[null,null,null,null,5338,"38_26/10/2019 10:52:31 AM","2019-01-01","Defect","Ship Staff","Ship Staff Insp.","FO Supply pump #2 for ME & AE started leaking from Mechanical seal","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Supply pump leak started after changing over to LSMGO. Dismantled pump, seal lapping carried out and leak rectified.","2019-01-02","","Completed","2019-01-02","No","No","No","Internal"]
[null,null,null,null,5339,"38_26/10/2019 10:54:54 AM","2019-01-01","Defect","Ship Staff","Ship Staff Insp.","Deck seal Steam line leaking after increasing steam pressure","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","Equipment Related","8.27","Medium","","","Leakage started after frozen return line cleared and raised steam pressure. Line removed / repaired and fixed back.","2019-01-02","","Completed","2019-01-02","No","No","No","Internal"]
[null,null,null,null,5340,"38_26/10/2019 10:56:25 AM","2019-01-01","Defect","Ship Staff","Ship Staff Insp.","Leakages of LSMGO from Unit 2, 4, 5, 7 Puncture valves and Shock absorber of Unit #3, #4, #6 ","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Leakages started after changing over to LSMGO in ECA area. All leaking puncture valves O. Rings replaced. Unit #7 Puncture valve replaced. Shock absorber in place overhauled","2019-01-02","","Completed","2019-01-02","No","No","No","Internal"]
[null,null,null,null,5327,"38_26/10/2019 10:32:02 AM","2019-01-02","Defect","Ship Staff","Ship Staff Insp.","Air valve for Testing Cargo sea chest integrity not holding","Miscellaneous","Structural Condn. / WT integrity ","Equipment Related","","","","","Replaced valve","2019-01-02","","Completed","2019-01-02","No","No","No","Internal"]
[null,null,null,null,5334,"38_26/10/2019 10:44:12 AM","2019-01-02","Defect","Ship Staff","Ship Staff Insp.","AE inlet Flow meter leaking and also not working","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","By pass valve opened, Removed Flow meter, found freezed bearings with Gear, Boxed up back. New Flow meter to supply. Ridgebury planning to supply all new Flow meters","2019-01-03","","Completed","2019-01-02","No","No","No","Internal"]
[null,null,null,null,5335,"38_26/10/2019 10:46:02 AM","2019-01-02","Defect","Ship Staff","Ship Staff Insp.","Sewage Vacuum System not working, suspect chocking","Miscellaneous","Structural Condn. / WT integrity ","Equipment Related","10.32","Very High","","","Removed Port side line and cleared, system made operational.","2019-01-03","","Completed","2019-01-03","No","No","No","Internal"]
[null,null,null,null,5336,"38_26/10/2019 10:47:47 AM","2019-01-02","Defect","Ship Staff","Ship Staff Insp.","Sewage dosing Pump in operative","Miscellaneous","Structural Condn. / WT integrity ","Equipment Related","10.32","Very High","","","Sewage dosage pump dismantled, found damaged diapharagm, Diapharagm canibalised from other spares and pump made operational","2019-01-03","","Completed","2019-01-03","No","No","No","Internal"]
[null,null,null,null,5337,"38_26/10/2019 10:49:18 AM","2019-01-02","Defect","Ship Staff","Ship Staff Insp.","Stbd Gangway line leaking","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","Equipment Related","5.47","Medium","","","Gangway Line removed and fabricated new and fixed in place","2019-01-02","","Completed","2019-01-02","No","No","No","Internal"]
[null,null,null,null,5333,"38_26/10/2019 10:42:34 AM","2019-01-03","Defect","Ship Staff","Ship Staff Insp.","Stbd Boiler not Firing","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Boiler Flow switch found faulty, same replaced. Inlet three way valve actuator found defective, same overhauled.  FD fan Parameter changed ton Risier and same changed to lowering after consultation with Maker's representative","2019-01-03","","Completed","2019-01-03","No","No","No","Internal"]
[null,null,null,null,5332,"38_26/10/2019 10:41:12 AM","2019-01-04","Defect","Ship Staff","Ship Staff Insp.","Port IG Fan Motor Drive End side Bearing freezed","Inert Gas","Structural Condn. / WT integrity ","Equipment Related","10.32","Very High","","","Motor replaced with Spare motor, removed Motor overhauled and kept as spare","2019-01-10","","Completed","2019-01-08","No","No","No","Internal"]
[null,null,null,null,5330,"38_26/10/2019 10:37:54 AM","2019-01-06","Defect","Ship Staff","Ship Staff Insp.","Boiler Main feed Pump #1 Leaking from Seal","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Boiler feed pump Seal Replaced with Spare, Pump tested, all satisfactory","2019-01-10","","Completed","2019-01-09","No","No","No","Internal"]
[null,null,null,null,5193,"38_2019-10-24 18:05:31.000","2019-01-11","Defect","Ship Staff","Ship Staff Insp.","AC Plant not starting, found Transformer Burnt","E/R - Aux. Mach.,Critical Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Make shift arrangement made by Giving 220 volts in put from outside. Requisition for transformer raised","2019-01-31","","Completed","2019-01-18","No","No","No","Internal"]
[null,null,null,null,5326,"38_26/10/2019 10:30:10 AM","2019-01-12","Defect","Ship Staff","Ship Staff Insp.","Fresh water Line inlet to FWG holed, leaking","E/R - Pipes/ valves & fittings","General Appearance","Equipment Related","10.32","Very High","","","Pipe removeda nd welded, Fixed in place and system in use without any leak","2019-01-12","","Completed","2019-01-12","No","No","No","Internal"]
[null,null,null,null,5328,"38_26/10/2019 10:34:27 AM","2019-01-12","Defect","Ship Staff","Ship Staff Insp.","1C PV Valve found leaking","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.31","High","","","Replaced with spare O/H PV valve","2019-01-16","","Completed","2019-01-14","No","No","No","Internal"]
[null,null,null,null,5325,"38_26/10/2019 10:27:41 AM","2019-01-14","Defect","Ship Staff","Ship Staff Insp.","Air Compressor #1 eaking from cylinder head. ","E/R - Aux. Mach.","Structural Condn. / WT integrity ","Equipment Related","10.32","Very High","","","Cylinder head Gasket replaced with new. System checked, all satisfactory.","2019-01-15","","Completed","2019-01-15","No","No","No","Internal"]
[null,null,null,null,5182,"38_24/10/2019 5:06:55 PM","2019-01-15","Defect","Ship Staff","Ship Staff Insp.","FW v/v found leaking portside Upper deck entrance","Deck - Pipe / Fittings","Eng. / Strg. Comp.","Equipment Related","11.4","Very High","","","Replaced v/v","2019-01-17","","Completed","2019-01-16","No","No","No","Internal"]
[null,null,null,null,5183,"38_24/10/2019 5:09:09 PM","2019-01-16","Non Conformity","Ship Staff","Ship Staff Insp.","Air v/v near 3C found not holding","E/R - Air Comp.,Deck - Pipe / Fittings","Eng. / Strg. Comp.","Equipment Related","11.4","Very High","","","Valve replaced","2019-01-17","","Completed","2019-01-17","No","No","No","Internal"]
[null,null,null,null,5181,"38_24/10/2019 5:02:57 PM","2019-01-18","Defect","Ship Staff","Ship Staff Insp.","IG branch (1 C/P/S, 2 C/P/S, 3C ) valves hard to operate","Critical Equip.,Inert Gas","Cargo / Ballast Systems","Equipment Related","8.19","High","","","O/H of gearbox carried out, Greasing done.","2019-01-31","","Completed","2019-01-29","No","No","No","Internal"]
[null,null,null,null,5185,"38_24/10/2019 4:54:49 PM","2019-01-28","Breakdown","Ship Staff","Ship Staff Insp.","Port Side IG blower motor bearings damaged and excessive vibration from Fan. ","Inert Gas","Cargo / Ballast Systems","Equipment Related,Human Error","10.32","Very High","","","Motor opened and found bearing casing worn out and impeller requires balancing. Landed ashore, motor and impeller reapired by NICO Fujairah. After receiving onboard, fitted back. Changed resilience mountings. During trial observed no change in vibration. Job included in REFMAN. Requisition raised for new Imeller.","2019-04-30","REAG190066","Completed","2019-06-02","No","No","No","Internal"]
[null,null,null,null,5196,"38_24/10/2019 4:56:48 PM","2019-01-28","Non Conformity","Ship Staff","Ship Staff Insp.","Hyd leak on pipe line going to Hyd. Box no.1 on Main deck","Deck - Machinery","Cargo / Ballast Systems","Equipment Related","11.4","Very High","","","To be rectified by ship staff","2019-03-10","","Completed","2019-02-06","No","No","No","Internal"]
[null,null,null,null,5190,"38_24/10/2019 5:57:04 PM","2019-01-31","Defect","Ship Staff","Ship Staff Insp.","During Crankcase inspection found piston cooling drain pipe cracked","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","After advice from Maker and office, Drain channel removed and welded in workshop , fixed back, all satisfactory.","2019-05-02","","Completed","2019-04-02","No","No","No","Internal"]
[null,null,null,null,5194,"38_24/10/2019 6:26:47 PM","2019-02-02","Non Conformity","Ship Staff","Ship Staff Insp.","Manifold drip tray drain valve not holding, need overhauling","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.41","Medium","","","Valve overhauled and paint, particles removed/cleared and valve fixed back, tested holding good","2019-02-18","","Completed","2019-02-17","No","No","No","Internal"]
[null,null,null,null,5191,"38_24/10/2019 5:58:44 PM","2019-02-03","Defect","Ship Staff","Ship Staff Insp.","FWG inlet Sea water line holed","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","11.4","Very High","","","Line removed and welded in workshop. All satisfactory.","2019-02-04","","Completed","2019-02-04","No","No","No","Internal"]
[null,null,null,null,5184,"38_24/10/2019 5:16:40 PM","2019-02-05","Defect","Ship Staff","Ship Staff Insp.","Hydraulic line (for valve CO622F - opening side) under hydraulic box no. 3 found pin hole leak","Cargo Mach.,Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","10.17","Very High","","","Line dismantle armato coupling fixed, tested no leak observed","2019-02-05","","Completed","2019-02-05","No","No","No","Internal"]
[null,null,null,null,5192,"38_24/10/2019 6:02:46 PM","2019-02-05","Defect","Ship Staff","Ship Staff Insp.","Scrubber primary Chamber body holed, required to repair by welding (Temporary Repair)","Inert Gas","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","After office approval Hot work carried out and repaired by doubler. Job added to REFMAN ","2019-02-06","","Completed","2019-02-06","No","No","No","Internal"]
[null,null,null,null,5187,"38_24/10/2019 5:47:31 PM","2019-02-06","Non Conformity","Ship Staff","Ship Staff Insp.","Fire hydrant in Pump rooom bottom platform stbdside found leaking","LSA / FFA","Safety / LSA / FFA","Equipment Related","12.15","High","","","Fire hydrant replace and checked no leak observed","2019-02-06","","Completed","2019-02-06","No","No","No","Internal"]
[null,null,null,null,5188,"38_24/10/2019 5:49:21 PM","2019-02-09","Defect","Ship Staff","Ship Staff Insp.","Gangway air motor not working","Deck - Machinery","ISM Related","Equipment Related","5.47","Medium","","","Over hauling done, found damage rotor blade damge, replaced rotor blade. Requisition raised. ","2019-02-09","REAG190056","Completed","2019-02-09","No","No","No","Internal"]
[null,null,null,null,5189,"38_24/10/2019 5:51:22 PM","2019-02-11","Defect","Ship Staff","Ship Staff Insp.","Reducer surface presentation flange not in good condition, paint found cracked and surface un even.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.41","Medium","","","Buffing carried out and surface of the presentation flange made even and old crack paint removed ","2019-02-11","","Completed","2019-02-11","No","No","No","Internal"]
[null,null,null,null,5320,"38_26/10/2019 10:06:50 AM","2019-02-11","Defect","Ship Staff","Ship Staff Insp.","NO.1 IG FAN too much vibration when running.","Inert Gas","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","IG FAN to change with old spare and test","2019-04-15","REAG190113","Completed","2019-04-30","No","No","No","Internal"]
[null,null,null,null,5195,"38_24/10/2019 6:29:10 PM","2019-02-13","Defect","Ship Staff","Ship Staff Insp.","Gangway stbd side shifting wire rope found damage.","Deck - Machinery","ISM Related","Equipment Related","5.47","Medium","","","Shifting wire replaced with new wire rope","2019-02-13","","Completed","2019-02-13","No","No","No","Internal"]
[null,null,null,null,5323,"38_26/10/2019 10:15:32 AM","2019-02-15","Defect","Ship Staff","Ship Staff Insp.","Anchor wash pipe clogged with heavy rust particles including 3 nos. of nozzle's on portside.","Miscellaneous","Structural Condn. / WT integrity ","Equipment Related","","","","","Anchor wash pipe in bosun store and valve on top dismantle, cleared rust particles and cleared, pipe and valve fixed back. Test no leaksand anchor washing all nozzle clear.","2019-02-23","","Completed","2019-02-22","No","No","No","Internal"]
[null,null,null,null,5198,"38_2019-10-25 18:37:56.000","2019-02-18","Non Conformity","Ship Staff","Ship Staff Insp.","Manifold drip tray drain valve found leaking","Cargo Mach.,Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.67","High","","","Drain valve over hauled, fixed back and tested, holding.","2019-02-19","","Completed","2019-02-19","No","No","No","Internal"]
[null,null,null,null,5324,"38_26/10/2019 10:24:43 AM","2019-02-20","Defect","Ship Staff","Ship Staff Insp.","STBD Gangway shifting wire found damage during routine inspection.","Miscellaneous","Structural Condn. / WT integrity ","Equipment Related","5.47","Medium","","","Shifting wire replaced with new wire.","2019-02-20","","Completed","2019-02-20","No","No","No","Internal"]
[null,null,null,null,5322,"38_26/10/2019 10:12:06 AM","2019-02-22","Defect","Ship Staff","Ship Staff Insp.","Stbdside anchor wash pipe 2 nozzle clogged with heavy rust particles","Miscellaneous","Structural Condn. / WT integrity ","Equipment Related","","","","","Pipe dismantle and cleared all clogged particles, pipe fitted back gasket renewed and tested no leaks and anchor washing all nozzle clear.","2019-02-24","","Completed","2019-02-24","No","No","No","Internal"]
[null,null,null,null,5321,"38_26/10/2019 10:08:21 AM","2019-02-23","","Ship Staff","Ship Staff Insp.","Hyd. Isolation valve for ODME Overboard discharge valve CO 612 found leaking from gland packing.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.18","High","","","Hyd isolation valve opened from gland packing and O'ring renewed, no leak observed.","2019-02-23","","Completed","2019-02-23","No","No","No","Internal"]
[null,null,null,null,5314,"38_26/10/2019 9:56:55 AM","2019-03-04","Defect","Ship Staff","Ship Staff Insp.","Cargo tanks many IG isolation valves leaking. Same to identify and rectify. Requisition is raised.","Inert Gas","Cargo / Ballast Systems","Equipment Related","8.19","High","","","Done by ship staff","2019-04-15","REAG190124","Completed","2019-05-13","No","No","No","Internal"]
[null,null,null,null,5313,"38_26/10/2019 9:55:00 AM","2019-03-15","Defect","Ship Staff","Ship Staff Insp.","ME Camshaft LO pump no.2 seal leaking. Spare new seal not available onboard. Requisition raiseD.presently repaired with old seal.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Pump overhauled,mechanical seal renewed.","2019-05-30","REAG190129","Completed","2019-05-28","No","No","No","Internal"]
[null,null,null,null,5315,"38_26/10/2019 9:58:49 AM","2019-03-15","Defect","Ship Staff","Ship Staff Insp.","Stbd/Port Windlass brake arrangement universal coupling in very poor condition.","Deck - Mooring Machinery","Mooring","Equipment Related","9.2","Very High","","","To be done in DD. Requisition to raise.","2019-04-15","","Completed","2019-05-02","No","No","No","Internal"]
[null,null,null,null,5319,"38_26/10/2019 10:05:08 AM","2019-03-17","Defect","Ship Staff","Ship Staff Insp.","Vaccum condenser inlet valve stuck in open position. Same to open and free in DD","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","10.32","Very High","","","To be done in DD. ","2019-04-15","","Completed","2019-04-30","No","No","No","Internal"]
[null,null,null,null,5318,"38_26/10/2019 10:03:20 AM","2019-03-22","Defect","Ship Staff","Ship Staff Insp.","Economizer feed water pump No.2 Aft seal leaking.. Requisition raiseD.presently repaired with old seal.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Requisition raised. Awaiting spares","2019-04-15","REAG190127","Completed","2019-04-30","No","No","No","Internal"]
[null,null,null,null,5317,"38_26/10/2019 10:01:41 AM","2019-03-26","","Ship Staff","Ship Staff Insp.","COP Main steam valve leaking.Same to open and overhaul in DD","Cargo Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","To be done in DD. ","2019-04-15","","Completed","2019-04-30","No","No","No","Internal"]
[null,null,null,null,5316,"38_26/10/2019 10:00:23 AM","2019-03-29","Defect","Ship Staff","Ship Staff Insp.","FWG Ejector pump discharge line leaking,Same to be renewed in DD","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","To be done in DD. ","2019-04-15","","Completed","2019-04-30","No","No","No","Internal"]
[null,null,null,null,7767,"38_Fri Oct 25 2019 19:24:23 GMT+0000 (Coordinated Universal Time)","2019-05-05","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","B deck vacuum toilet in operational, spares to order & rectify the toilet seat","Accommodation","MLC Related","Equipment Related","11.13","Low","","","RO RAISED FOR NEW TOILET SEAT AND FLEXIBLE CONNECTIONS/BENDS (REPEATED DEFECT IN LIST)","2019-12-31","REAG 190165","Completed","2020-08-05","No","No","No","Internal"]
[null,null,null,null,5210,"38_2019-10-25 19:07:26.000","2019-05-05","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Sewage outlet pipe line modification to aft peak tank on deck to be fabricated.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Flange with fire hose connection fabricated and kept ready going to aft peek tank on deck ","2019-09-30","","Completed","2019-09-27","No","No","No","Internal"]
[null,null,null,null,5234,"38_2019-10-25 19:43:44.000","2019-05-05","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","2 in no. nakakita temp/pressure controller to be made operational after fitting/fabricating sensor pocket in the fuel/Lube oil pipeline   ","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","PIPE FABRICATION TO BE CARRIED OUT AFTER JOB COMPLETION OF PBT","2019-09-30","","Completed","2019-09-10","No","No","No","Internal"]
[null,null,null,null,5268,"38_25/10/2019 10:03:32 PM","2019-05-05","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","All the jobs/services on deck & Engine to be updated in PAL PMS with relevant work done reports, photos, and service report as applicable.","Documentation","Cert. & Docu.","Human Error","10.12","Very High","","","VESSEL IN PROCESS OF UPDATING IN PAL","2019-06-20","","Completed","2019-07-01","No","No","No","Internal"]
[null,null,null,null,5269,"38_25/10/2019 10:05:14 PM","2019-05-05","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ER housing keeping, painting etc. to be carried out & prepare the vessel for upcoming vetting.","Miscellaneous","General Appearance","Human Error","10.29","Medium","","","CLEANING AND PAINTING OF ENGINE ROOM IN PROGRESS","2019-05-06","","Completed","2019-06-10","No","No","No","Internal"]
[null,null,null,null,5291,"38_26/10/2019 12:26:37 AM","2019-05-05","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Bilge primary tank remaining pipe fitting jobs to be carried out & system to be made operational, class approved piping diagram received to be laminated & posted near the pump.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","WORK IN PROGRESS, COMPLETION EXPECTED IN 3-4 DAYS","2019-06-20","","Completed","2019-05-06","No","No","No","Internal"]
[null,null,null,null,5292,"38_26/10/2019 12:30:09 AM","2019-05-05","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp."," All IMO safety symbols on deck as well as in ER to be checked, damaged ones to be replaced with new one.","LSA / FFA","Safety / LSA / FFA","Inappropriate Procedure","5.31","High","","","JOB COMPLETED","2019-05-21","","Completed","2019-06-11","No","No","No","Internal"]
[null,null,null,null,5293,"38_26/10/2019 12:32:50 AM","2019-05-05","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","cargo Manifold crossover valves leak test to carry out after loading operations","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.18","High","","","JOB COMPLETED, NO LEAKS OBSERVED","2019-06-15","","Completed","2019-06-05","No","No","No","Internal"]
[null,null,null,null,5294,"38_26/10/2019 12:35:59 AM","2019-05-05","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Both Mid ship crane angle indictor rod to be fitted & angle paint marking to be carried out.","Deck - Machinery","Cargo / Ballast Systems","Equipment Related","8.5","Very High","","","JOB COMPLETED","2019-05-20","","Completed","2019-05-16","No","No","No","Internal"]
[null,null,null,null,5295,"38_26/10/2019 12:39:10 AM","2019-05-05","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Port side provision crane hook safety latch with spring to be fabricated ","Deck - Machinery","Cargo / Ballast Systems","Equipment Related","8.5","Very High","","","JOB COMPLETED,SAFETY LATCHES FITTED WHERE MISSING ON CRANE HOOKS","2019-05-06","","Completed","2019-05-15","No","No","No","Internal"]
[null,null,null,null,5296,"38_26/10/2019 1:17:31 AM","2019-05-05","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ER aft bilge well has oil tracers, same to be cleaned. spring loaded steering room drain line leading to be aft bilge well to be operated & make sure all the effluent & oil traces are drained & collected in bucket.","Miscellaneous","Eng. / Strg. Comp.","Human Error","10.29","Medium","","","JOB COMPLETED","2019-05-15","","Completed","2019-05-14","No","No","No","Internal"]
[null,null,null,null,5297,"38_26/10/2019 1:19:15 AM","2019-05-05","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","steering room bilge well to be cleaned & free of oil traces","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","JOB COMPLETED","2019-05-12","","Completed","2019-05-10","No","No","No","Internal"]
[null,null,null,null,5298,"38_26/10/2019 1:21:25 AM","2019-05-05","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","All the ER DB tanks sounding & pipes springs to be fitted back, fire hoses & tightening clamp/handles to be kept back in place.","Miscellaneous","Eng. / Strg. Comp.","Human Error","10.32","Very High","","","JOB COMPLETED","2019-06-05","","Completed","2019-05-10","No","No","No","Internal"]
[null,null,null,null,5299,"38_26/10/2019 1:23:33 AM","2019-05-05","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","All the old /unused spares to be secured at respective locations & updated in PAL as applicable.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Behaviour Based","10.29","Medium","","","JOB COMPLETED","2019-05-11","","Completed","2019-05-15","No","No","No","Internal"]
[null,null,null,null,5300,"38_26/10/2019 1:26:03 AM","2019-05-05","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Main engine performance test & Speed fuel consumption test both in ballast & loaded condition to be carried out at various RPM in order to compare with sea trial report & record keeping.","E/R - Main Engine","Eng. / Strg. Comp.","External Factors","10.7","Medium","","","JOB COMPLETED","2019-05-06","","Completed","2019-05-11","No","No","No","Internal"]
[null,null,null,null,5301,"38_26/10/2019 1:27:43 AM","2019-05-05","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ME Lube oil feed rate to be reduced to normal level of 0.9-to 1 gm/kwhr after 20 hrs of running IN operation","E/R - Main Engine","Eng. / Strg. Comp.","Human Error","10.7","Medium","","","JOB COMPLETED","2019-06-05","","Completed","2019-05-06","No","No","No","Internal"]
[null,null,null,null,5302,"38_26/10/2019 1:29:29 AM","2019-05-05","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ME scavenge space & crankcase inspection to be carried out at first available opportunity & report to be submitted to office","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.12","Very High","","","JOB COMPLETED","2019-06-15","","Completed","2019-05-21","No","No","No","Internal"]
[null,null,null,null,5303,"38_26/10/2019 1:31:06 AM","2019-05-05","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Both Boiler & jacket cooling water chemicals to be dosed to bring the parameters to maker recommended levels. ","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","JOB COMPLETED","2019-08-05","","Completed","2019-05-10","No","No","No","Internal"]
[null,null,null,null,5304,"38_26/10/2019 1:33:35 AM","2019-05-05","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","6 in no. panama chocks outside grooving marks to be filled with welding electrodes.","Deck - Pipe / Fittings","Mooring","Equipment Related","9.19","Low","","","JOB COMPLETED","2019-05-15","","Completed","2019-05-11","No","No","No","Internal"]
[null,null,null,null,5305,"38_26/10/2019 1:35:18 AM","2019-05-05","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Testing of safety devices post DD 14.37.01.001.01 checklist to be completed & forward to office.","Documentation","Cert. & Docu.","Knowledge Based","5.27","Medium","","","CHECKLIST COMPLETED AND SENT TO OFFICE/UPDATED AS ONE TIME JOB IN PAL","2019-05-25","","Completed","2019-05-09","No","No","No","Internal"]
[null,null,null,null,5306,"38_26/10/2019 1:36:57 AM","2019-05-05","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Slop tank steam coils broken wheel to change with new supplied wheels","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.15","High","","","JOB COMPLETED","2019-05-20","","Completed","2019-05-19","No","No","No","Internal"]
[null,null,null,null,5307,"38_26/10/2019 1:38:46 AM","2019-05-05","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","All the ballast/cargo tank Man holes & domes to be covered & tightened with new gaskets after carrying out tank inspection.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","2.16","Medium","","","JOB COMPLETED","2019-05-10","","Completed","2019-05-09","No","No","No","Internal"]
[null,null,null,null,5308,"38_26/10/2019 2:18:14 AM","2019-05-05","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","All the new deck hyd pipe & steam pipe fabricated, U clamp to loosen & Teflon gaskets to be inserted.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","11.4","Very High","","","JOB COMPLETED","2019-05-25","","Completed","2019-05-10","No","No","No","Internal"]
[null,null,null,null,5309,"38_26/10/2019 2:20:13 AM","2019-05-05","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Port side crane bearing inspection door to be fabricated with new one.","Deck - Machinery","Cargo / Ballast Systems","Equipment Related","8.5","Very High","","","JOB COMPLETED","2019-05-20","","Completed","2019-05-13","No","No","No","Internal"]
[null,null,null,null,5310,"38_26/10/2019 2:22:45 AM","2019-05-05","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Bosun store light switch near speed log sensor to be fitted back.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Human Error","11.1","High","","","SWITCH FITTED BACK IN PLACE","2019-05-15","","Completed","2019-05-31","No","No","No","Internal"]
[null,null,null,null,5311,"38_26/10/2019 2:24:58 AM","2019-05-05","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","All the sounding pipes caps ballast tk, bunker tank, fire hoses, life buoys etc. to be fitted back on its place","Deck - Pipe / Fittings","General Appearance","External Factors","2.16","Medium","","","COMPLETED PACING BACK L/BOUYS,SOUNDING CAPS,FIRE HOSES ETC AFTER DD","2019-05-07","","Completed","2019-05-09","No","No","No","Internal"]
[null,null,null,null,5312,"38_26/10/2019 2:26:49 AM","2019-05-05","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Housekeeping in accommodation, common scape toilets etc. to be upgraded","Accommodation","General Appearance","External Factors","11.13","Low","","","ACCOMODATION CLEANING COMPLETED,PUBLIC TOILETS AND AREAS CLEANED","2019-05-15","","Completed","2019-05-14","No","No","No","Internal"]
[null,null,null,null,5255,"38_2019-10-25 20:43:26.000","2019-05-16","Defect","Ship Staff","Ship Staff Insp.","Issues with Vacuum Toilet system,not working properly.Upper Dk and B Dk toilets blanked","Miscellaneous","MLC Related","Equipment Related","11.13","Low","","","Requisition raised and awaiting spares","2019-06-30","REAG 190165","Completed","2019-07-10","No","No","No","Internal"]
[null,null,null,null,null,"38_25/10/2019 6:31:14 PM","2019-05-16","Defect","Ship Staff","Ship Staff Insp.","Main engine and Diesel generator JCW controllers not functional","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Main Engine controller was  calibrated and linkage was connected to 3-way valve,presently oprated satisfactiry at AUTO mode.","2019-12-31",null,"Completed","2020-11-18","No",null,null,"Internal"]
[null,null,null,null,5230,"38_2019-10-25 19:38:05.000","2019-05-17","Defect","Ship Staff","Ship Staff Insp.","Fwd LT cooler Plates leaking from fresh water side.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Temporary repair to be carried out at first opportunity and to observe the leak.","2019-09-18","","Completed","2019-09-05","No","No","No","Internal"]
[null,null,null,null,5278,"38_25/10/2019 10:28:30 PM","2019-05-17","Defect","Ship Staff","Ship Staff Insp.","Air Conn no.2 unit, coupling damaged","E/R - Air Comp.","MLC Related","Equipment Related","10.32","Very High","","","Requisition raised and awaiting spares","2019-06-18","REAG190174","Completed","2019-06-23","No","No","No","Internal"]
[null,null,null,null,5161,"38_25/10/2019 6:27:33 PM","2019-05-18","Non Conformity","Ship Staff","Ship Staff Insp.","Alarm Monitoring System associated with  LCU 7,8,9 & 10 not showing the parameter values","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.2","Low","","","After joinjing, inspected, found working","2019-12-31","","Completed","2020-06-21","No","No","No","Internal","will arrange technician at convenient port, understand presently no operational issues due to it."]
[null,null,null,null,5163,"38_25/10/2019 6:32:56 PM","2019-05-18","Defect","Ship Staff","Ship Staff Insp.","ME Crank case relief door leaking.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Crank case relief door opened and found O'ring in good condition, gasket drain hole was not made the same made and boxed back.","2019-11-15","","Completed","2019-11-04","No","No","No","Internal","Pls revert with progress status for same."]
[null,null,null,null,5235,"38_2019-10-25 19:45:04.000","2019-05-18","Defect","Ship Staff","Ship Staff Insp.","Main engine fwd cover, holding encoder leaking.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Re tightning of cover carried out 26/08/2019 but still leaking. Job can be carried out at anchorage as the lower hafl has to be removed and checked.","2019-09-15","","Completed","2019-07-09","No","No","No","Internal"]
[null,null,null,null,5245,"38_2019-10-25 20:25:46.999","2019-05-18","Defect","Ship Staff","Ship Staff Insp.","Fwd LT cooler sea water inlet valve not operative (partially operates in open & close position)","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Valve renewed","2019-09-16","","Completed","2019-08-25","No","No","No","Internal"]
[null,null,null,null,5264,"38_2019-10-25 21:55:58.000","2019-05-18","Defect","Ship Staff","Ship Staff Insp.","Engine room Signal light column near hot well","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.37","Medium","","","PCB should be replaced with the new one.Requisition raised and awaiting spares","2019-06-13","REAG190191","Completed","2019-07-14","No","No","No","Internal"]
[null,null,null,null,5265,"38_2019-10-25 21:57:55.000","2019-05-18","Defect","Ship Staff","Ship Staff Insp.","Basic hand tools not available","Miscellaneous","General Appearance","Equipment Related","","","","","Requisition raised and awaiting spares","2019-06-15","REAG190187","Completed","2019-07-14","No","No","No","Internal"]
[null,null,null,null,5270,"38_2019-10-25 22:07:08.000","2019-05-18","Defect","Ship Staff","Ship Staff Insp.","D/G KRAL monitoring control unit defective","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Will be replaced under guarantee claim.","2019-06-25","","Completed","2019-07-02","No","No","No","Internal"]
[null,null,null,null,5160,"38_25/10/2019 6:22:46 PM","2019-05-20","Non Conformity","Ship Staff","Ship Staff Insp.","Ballast tank/draft gauge gauging system giving erratic reading","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.12","Medium","","","Same Job reported on Aug-2019 as Ballast draft Gauge system malfunction.","2020-01-31","","Completed","2020-11-10","No","No","No","Internal","You indicated that you planned to carry out calibration in Mid Sept 2019.  Was this done?  If yes, we await your response.\n \n"]
[null,null,null,null,5225,"38_2019-10-25 19:31:08.000","2019-05-20","Defect","Ship Staff","Ship Staff Insp.","Incinerator Sludge burning not steady","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Investigation in progress.","2019-09-30","","Completed","2019-09-13","No","No","No","Internal"]
[null,null,null,null,5226,"38_2019-10-25 19:32:41.000","2019-05-20","Defect","Ship Staff","Ship Staff Insp.","Main air compressor taking too long time to top-up the bottle\n\n (19~26bar took 45minutes with each compressor)","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Cleaning and overhaul of compressor valves in progress.","2019-09-30","","Completed","2019-09-12","No","No","No","Internal"]
[null,null,null,null,5276,"38_25/10/2019 10:25:08 PM","2019-05-20","Defect","Ship Staff","Ship Staff Insp.","Fire alarm monitoring system zone 12 call point not functional","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.35","Medium","","","Cable should be checked and need to change the MCP","2019-10-06","REAG190189","Completed","2019-06-28","No","No","No","Internal"]
[null,null,null,null,5289,"38_25/10/2019 10:52:17 PM","2019-05-20","Defect","Ship Staff","Ship Staff Insp.","Alpha lubricator leaks at various joints","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","To be repaired at first opportunity of engine stoppage","2019-06-15","","Completed","2019-06-16","No","No","No","Internal"]
[null,null,null,null,5203,"38_25/10/2019 6:55:17 PM","2019-05-21","Defect","Ship Staff","Ship Staff Insp.","All three DG lube oil coolers leaking, gaskets to be renewed.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","All DG oil cooler leaks rectified.","2019-09-30","","Completed","2019-09-29","No","No","No","Internal"]
[null,null,null,null,5266,"38_25/10/2019 9:59:29 PM","2019-05-21","Defect","Ship Staff","Ship Staff Insp.","Main Engine under piston doors leaking from most units","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.19","Very High","","","Leak to be arrested by sealing the thread holes.","2019-06-15","","Completed","2019-07-15","No","No","No","Internal"]
[null,null,null,null,5267,"38_2019-10-25 22:00:51.999","2019-05-21","Defect","Ship Staff","Ship Staff Insp.","Appearance of M.E sump oil dark and sludgy but Analysis reports reflects in good condition","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.7","Medium","","","Purifier operation to be effective and under close monitoring.","2019-06-30","","Completed","2019-07-01","No","No","No","Internal"]
[null,null,null,null,5256,"38_2019-10-25 21:38:39.000","2019-05-22","Defect","Ship Staff","Ship Staff Insp.","M.E KRAL unit consumption not matching with tank sounding consumptions","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Communicated with Fleet 1 correspondence in regards is in progress.","2019-09-30","","Completed","2019-07-15","No","No","No","Internal"]
[null,null,null,null,5288,"38_25/10/2019 10:47:12 PM","2019-05-25","Defect","Ship Staff","Ship Staff Insp.","Workshop Airconn not operative","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","To Identify the cause and if required spare parts to be ordered. Job cancelled","2019-06-30","","Completed","2019-06-16","No","No","No","Internal"]
[null,null,null,null,5229,"38_2019-10-25 19:36:43.999","2019-05-27","Defect","Ship Staff","Ship Staff Insp.","ME LO Back wash candle filters and bypass filters getting clogged often. No spare filters on board for interchanging the filters in emergency.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.19","Very High","","","filter will be replaced at first opportunity. ","2019-09-20","","Completed","2019-09-01","No","No","No","Internal"]
[null,null,null,null,5290,"38_25/10/2019 10:53:34 PM","2019-05-27","Defect","Ship Staff","Ship Staff Insp.","Main engine unit no.7 fuel oil drain line holed","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Will be repaired at first opportunity of Engine stoppage.","2019-06-15","","Completed","2019-06-13","No","No","No","Internal"]
[null,null,null,null,5279,"38_25/10/2019 10:30:07 PM","2019-05-29","Defect","Ship Staff","Ship Staff Insp.","440V low insulation on fwd horn ","Elect. Mach. & Equip.","Navigation","Equipment Related","10.24","Low","","","Job will be attended , crossing Singapore straight ","2019-06-18","","Completed","2019-06-20","No","No","No","Internal"]
[null,null,null,null,5277,"38_25/10/2019 10:26:28 PM","2019-06-03","Defect","Ship Staff","Ship Staff Insp.","No spare fire detectors onboard (smoke, flame & heat).","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.39","Very High","","","Requisition raised and awaiting spares","2019-06-20","REAG190189","Completed","2019-06-18","No","No","No","Internal"]
[null,null,null,null,5271,"38_25/10/2019 10:16:12 PM","2019-06-05","Defect","Ship Staff","Ship Staff Insp.","HOSPITAL EXHAUST FAN IN-OPERATIONAL","Accommodation","MLC Related","Equipment Related","11.15","Low","","","RO RAISED FOR NEW EXHAUST FAN TO REPLACE THE FAULTY ONE","2019-06-14","REAG 195100","Completed","2019-07-06","No","No","No","Internal"]
[null,null,null,null,5280,"38_25/10/2019 10:31:34 PM","2019-06-05","Defect","Ship Staff","Ship Staff Insp.","Vapour recovery system oxygen sensor not operational","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.42","Medium","","","RO RAISED FOR NEW OXYGEN SENSOR TO REPLACE THE FAULTY ONE","2019-07-15","REAG190167","Completed","2019-06-22","No","No","No","Internal"]
[null,null,null,null,5165,"38_25/10/2019 6:36:57 PM","2019-06-15","Defect","Ship Staff","Ship Staff Insp.","Stbd Aft Capston motor not working","Deck - Machinery","Mooring","Equipment Related","","","","","Replaced control transformer with new one, clean terminal with electrosolve and sealed the junction box.","2020-01-31","","Completed","2020-11-17","No","No","No","Internal","What was the result of your investigation for zero insulation? Did you managed to find the problem?"]
[null,null,null,null,5241,"38_2019-10-25 20:10:26.000","2019-06-15","Defect","Ship Staff","Ship Staff Insp.","LIGHT SIGNAL COLUMN","Elect. Mach. & Equip.","Emgcy. Systems","Equipment Related","","","","","Job completed","2019-08-15","REAG190200","Completed","2019-08-20","No","No","No","Internal"]
[null,null,null,null,5242,"38_2019-10-25 20:13:29.000","2019-06-15","Defect","Ship Staff","Ship Staff Insp.","FWD BOSUN STORE INSULATION METER FAULTY","Elect. Mach. & Equip.","Cargo / Ballast Systems","Equipment Related","10.24","Low","","","Job completed ","2019-09-15","REAG190199","Completed","2019-08-29","No","No","No","Internal"]
[null,null,null,null,10093,"38_Tue Jan 21 2020 12:10:28 GMT+0000","2019-06-18","Observation","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","AROUND 60% NUMBER OF U BOLTS OF THE MAIN PIPELINES OF COW LINE,FIRE LINE,FOAM LINE & ELECTRIC CONDUIT ON THE MAIN DECK WERE CORREDED GENERALLY & POOR CONDITION.","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.5","Medium","","","Cause\nThe vessel has been carrying out the Hydro Blasting of all U-Bolts on main deck as per planned schedule as noted by the inspector and all the U-Clamps from Forward to Midship area had been blasted and re-painted. \nCorrective Action\nWe wish to advise that the job of Hydro Blasting and painting the U-Bolts and Clamps  completed by 31st July 2019","2019-07-20","","Completed","2019-07-31","No","No","No","External","well noted"]
[null,null,null,null,5159,"38_2019-10-25 21:46:14.999","2019-06-19","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","q. Gymnasium.","Miscellaneous","Crew Management","Equipment Related","11.13","Low","","","Old non-working Gym item to be disposed, Broken chairs to be removed/disposed. Make proper arrangement in side the Gym area.","2019-07-15","","Completed","2019-07-09","No","No","No","Internal"]
[null,null,null,null,5166,"38_25/10/2019 6:39:26 PM","2019-06-19","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","No.2 Main air compressor. ","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Resilent mountings renewed","2019-12-31","REAG 190248","Completed","2020-01-28","No","No","No","Internal","spares already supplied in Fujairah, please update on the job progress"]
[null,null,null,null,5236,"38_2019-10-25 19:49:40.000","2019-06-19","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ECDIS (Transas NAVISALIOR 4000).","Navigation - ECDIS","Navigation","Equipment Related","7.14","Medium","","","1. It was reported that sometimes both ECDISs are slow and hangs up. There must be old Log filed and route filed inside the ECDIS since long time which reduce the HDD capacity.2nd Officer need to delete all old Route files and Log filed and re-boot the ECDIS and revert with result.\n\n2.    NAVTOR Box is not online with both ECDIS.Vessel need to connect one LAN cable form NAVTOR box and connect this LAN cable to Transas ECDIS NETWORK Switch. After connecting this LAN Cable follow up with NAVTOR SUPPORT team and configure same and make both ECDIS online with NAVTOR BOX.","2019-09-15","","Completed","2019-08-19","No","No","No","Internal"]
[null,null,null,null,5240,"38_2019-10-25 20:06:37.000","2019-06-19","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","l. MF/HF coupler unit and antenna.","Elect. Mach. & Equip.","Communication","Equipment Related","11.1","High","","","Job completed ","2019-08-15","","Completed","2019-08-24","No","No","No","Internal"]
[null,null,null,null,5243,"38_2019-10-25 20:15:40.000","2019-06-19","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","d. ER Workshop fire curtain for welding area. ","Miscellaneous","Eng. / Strg. Comp.","Inappropriate Procedure","","","","","ER Workshop fire curtain changed with new one.","2019-09-15","REAG190224","Completed","2019-08-27","No","No","No","Internal"]
[null,null,null,null,5252,"38_2019-10-25 20:39:39.000","2019-06-19","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","r. Oil record book.","Miscellaneous","Cargo / Ballast Systems","Human Error","2.11","Medium","","","There is some discrepancy in oil record book for transferring sludge/bilge oil to Slop tank (Port). Correct entry or revised entry to be make properly prior next SIRE or PSC observe this discrepancy.","2019-08-15","","Completed","2019-08-19","No","No","No","Internal"]
[null,null,null,null,5262,"38_2019-10-25 21:52:57.999","2019-06-19","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","p. Conference room.","Miscellaneous","General Appearance","Human Error","11.16","Low","","","Some of the old computers, spoilt one lying on conference room table including spare monitor. Only on internet computer is working.Remaining fault CPU to be removed from these area and monitors to be kept in IT room.ETO need to collect all IT stores and items and shift to IT spare locker. Many IT items segregated all over. Good items to be collected and keep it in one Place.","2019-07-15","","Completed","2019-07-07","No","No","No","Internal"]
[null,null,null,null,5263,"38_2019-10-25 21:54:25.000","2019-06-19","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","n. ME piston cooling flow sight glasses:","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.2","Low","","","All sight glasses are very dirty and unable to see piston cooling oil flow. Need to be cleaned for all engine units.","2019-07-15","","Completed","2019-07-15","No","No","No","Internal"]
[null,null,null,null,5274,"38_25/10/2019 10:22:02 PM","2019-06-19","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","o. CCR Gas sampling unit main vacuum pump.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","5.21","Medium","","","Main vacuum pump for gas sampling unit in CCR making some noise. It seems bearing noise form pump. Need to be rectified.","2019-07-15","","Completed","2019-06-28","No","No","No","Internal"]
[null,null,null,null,5275,"38_25/10/2019 10:23:29 PM","2019-06-19","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","f. AIS Pilot voltage plug missing form bridge front area.","Navigation - DGPS / EPFS / AIS","Navigation","Equipment Related","","","","","Understand AIS was upgraded recently, As per USCG requirement, there has to be 110 Volts power plug available next to AIS pilot plug.Explained to ETO and he has to install same next to AIS pilot plug for USCG requirement.","2019-07-15","","Completed","2019-06-28","No","No","No","Internal"]
[null,null,null,null,5281,"38_25/10/2019 10:33:33 PM","2019-06-19","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","k. Electrical cable bunch rubbing sharp metal cover.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.39","High","","","Out side the SG room, stbd side of ER, behind the boiler. One cable bunch touching/rubbing to cable tray cover top side and damaged. Need to insulate entire bunch and lift up little bit. Outer sheath of cable damaged and need to insulate same.","2019-07-15","","Completed","2019-06-22","No","No","No","Internal"]
[null,null,null,null,5282,"38_25/10/2019 10:34:56 PM","2019-06-19","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","j. SG Room, Rudder stock grounding cable","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.39","High","","","Rudder stock grounding cable is earthed on top part of SG room ceiling. This thick cable is touching/rubbing the rudder feedback unit rods/links. This might give wrong ridder feedback reading and may hamper steering. Need to shorten cable or make coil of one section and tie up with cable tie So it doesn’t touch or rub rudder feedback linkage.","2019-07-15","","Completed","2019-06-22","No","No","No","Internal"]
[null,null,null,null,5283,"38_25/10/2019 10:36:36 PM","2019-06-19","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","i. Accommodation surrounding lights:","Elect. Mach. & Equip.","General Appearance","Equipment Related","11.9","Low","","","1.    Accommodation surrounding tube lights are mixed up with LED and Fluorescent tubes. So mixed up with White day light and yellow illumination which  Doesn’t give good appearance. Some of the assembly (These are dual lights) mixed with LED and FL. This doesn’t fulfil LED conversation project.Raise the RO for next lot of LED tubes and replace all FL tubes to give proper white day light illumination. Also noticed that many LED tube lights holders are broken inside and handing inside the assembly. Vessel need to raise RO for tube light holder and replace same.\n\n2.    One of the tube light in funnel top casing area, de-fusser (Tube light cover) is missing. Need to be fixed properly.\n\n3.    One of the tube light assembly on top of the Deck store on stbd side poop deck, De-fuser was not fixed properly and it was handing. It was fitted during time of inspection but tube light assembly is not working. Need to repaired and make it operational.\n\n","2019-07-15","","Completed","2019-06-24","No","No","No","Internal"]
[null,null,null,null,5284,"38_25/10/2019 10:39:36 PM","2019-06-19","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","h. Electrical cable coaming:","Elect. Mach. & Equip.","ISM Related","Equipment Related","11.13","Low","","","1.    Upper deck electrical cable trunk (123) electrical coaming on floor is not filled up with electrical putty/cementing after passing new cable. This coaming is between accommodation to ER area, Which is consider as A-60 area. Cement on this coaming is broken for passing new cable and hot air Coming to this area from ER side. This will be very serious observation by PSC and SIRE side. Vessel need to fill up with cement or approved putty.\n\n2.    One cable coaming inside the purifier room to bottom section of Engine room is not filled up after passing new cable. Cements were broken and air wasPassing through out. This purifier room is consider as shield compartment and has to be filled up proper electrical putty and cement at first priority Prior PSC inspection. \n\n","2019-07-15","","Completed","2019-06-23","No","No","No","Internal"]
[null,null,null,null,5285,"38_25/10/2019 10:41:36 PM","2019-06-19","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","a. Wi-Fi in officers and crew recreational room","Accommodation","General Appearance","Equipment Related","11.13","Low","","","LAN cables are just dropped down and Wi-Fi unit is lying on floor. Must be fitted on wall and arrange the LAN cable properly.","2019-06-30","","Completed","2019-06-21","No","No","No","Internal"]
[null,null,null,null,5286,"38_25/10/2019 10:42:54 PM","2019-06-19","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","b. Tr. ETO cabin. ","Accommodation","General Appearance","Human Error","11.13","Low","","","Trainee ETO need to clean and arrange his cabin properly. It looks like garbage dumping area.","2019-06-20","","Completed","2019-06-20","No","No","No","Internal"]
[null,null,null,null,5287,"38_25/10/2019 10:44:23 PM","2019-06-19","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","e. LO sample analysis reports.","Miscellaneous","Cert. & Docu.","Human Error","10.7","Medium","","","Up to date LO and FO analysis reports to be filed it properly for future SIRE and PSC inspection. Some of the latest reports were missing form file during","2019-06-20","","Completed","2019-06-20","No","No","No","Internal"]
[null,null,null,null,5219,"38_2019-10-25 19:23:02.000","2019-06-20","Defect","Ship Staff","Ship Staff Insp.","MMC uti sr no 1467 power switch defective, unreliable.","Miscellaneous","Cargo / Ballast Systems","Equipment Related","8.2","Medium","","","Temporarily repaired. The MMC function verified Reading if Ullage and interface correct, Temp error +0.5*C, Audio and visual indicators function well. Compared With Calibrated MMC UTI.","2019-09-30","","Completed","2019-09-10","No","No","No","Internal"]
[null,null,null,null,5250,"38_2019-10-25 20:36:14.000","2019-06-20","Defect","Ship Staff","Ship Staff Insp.","APT Air vent pipe head float disc damage and holed, fwd 250A","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","11.7","High","","","Renewed with new spare rcvd on 17 aug 2019","2019-12-08","REAG190215","Completed","2019-08-23","No","No","No","Internal"]
[null,null,null,null,5251,"38_2019-10-25 20:38:06.000","2019-06-20","Defect","Ship Staff","Ship Staff Insp.","PORT PROVISION CRANE HOIST WIRE HAS TWO SHARP KINKS, WHICH RENDERS CONDEMNED AND SEVERILY AFFECTS OPERATIONS.","Deck - Machinery","ISM Related","Equipment Related","10.28","Low","","","Renewed with new wire rope rvcd 17 Aug 2019","2019-08-20","REAG19022","Completed","2019-08-23","No","No","No","Internal"]
[null,null,null,null,5260,"38_2019-10-25 21:49:27.999","2019-06-20","Defect","Ship Staff","Ship Staff Insp.","APT Air vent pipe head float disc damage and holed, aft 150A","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","11.7","High","","","REAG190215 raised on 25 Jun 2019 for spares","2019-12-07","REAG190215","Completed","2019-07-03","No","No","No","Internal"]
[null,null,null,null,5272,"38_25/10/2019 10:17:52 PM","2019-06-20","Defect","Ship Staff","Ship Staff Insp.","MMC uti sr no 1468 defective, unable to reading ullage/ interface","Miscellaneous","Cargo / Ballast Systems","Equipment Related","8.2","Medium","","","Sent ashore for service and returned, Satisfactory after repairs","2019-10-07","REAG195109","Completed","2019-07-01","No","No","No","Internal"]
[null,null,null,null,5273,"38_25/10/2019 10:20:16 PM","2019-06-20","Defect","Ship Staff","Ship Staff Insp.","PORT PROVISION CRANE HOIST WIRE HEAD BLOCK ONE NO. FROZEN.                                                                                                                                                HOISTING WIRE ROPE TWISTED","Deck - Machinery","General Appearance","Equipment Related","8.5","Very High","","","OPEN, REMOVED BLOCK SHAFT LUBRIACATED BUSH, INSPECTED, DERUSTED AND REFITTED TESTED  SATISFACTORY. OPENED THIMBLED END AND READJUSTED HOIST WIRE ROPE LAYING ON THE HEAD BLOCK TO CORRECT THE TWIST.","2019-10-07","","Completed","2019-07-03","No","No","No","Internal"]
[null,null,null,null,5218,"38_2019-10-25 19:21:01.999","2019-06-24","Defect","Ship Staff","Ship Staff Insp.","Minor hydraulic leak in box no 2 ,  from the hyrauilic block of valve CO 511.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","11.4","Very High","","","On investigation minor leak observed from the regulating valve of Intrinscically safe solenoid valve, opened and renew O-rings","2019-12-09","","Completed","2019-09-10","No","No","No","Internal"]
[null,null,null,null,5254,"38_2019-10-25 20:42:08.000","2019-06-24","Defect","Ship Staff","Ship Staff Insp.","Minor hydraulic leak in box no 1 ,  from the hyrauilic block ","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","11.4","Very High","","","Retightened block bolts , leak arrested","2019-08-15","","Completed","2019-08-03","No","No","No","Internal"]
[null,null,null,null,5259,"38_2019-10-25 21:47:37.000","2019-06-24","Defect","Ship Staff","Ship Staff Insp.","3c COT IGS valve in poor condition, integrity weak valve not holding.","Deck - Machinery","Cargo / Ballast Systems","Equipment Related","8.3","Very High","","","Replace valve with new spare","2019-12-07","","Completed","2019-07-04","No","No","No","Internal"]
[null,null,null,null,5261,"38_25/10/2019 9:50:57 PM","2019-06-24","Defect","Ship Staff","Ship Staff Insp.","BA 504 WBT 1port strip valve malfunction, does not close from CCR VRCS panel.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.18","High","","","Under investigation","2019-12-07","","Completed","2019-07-08","No","No","No","Internal"]
[null,null,null,null,5167,"38_25/10/2019 6:43:12 PM","2019-06-27","Defect","Ship Staff","Ship Staff Insp.","FGDS Pump room H2S 5 ppm and 10 ppm does not function","LSA / FFA","Safety / LSA / FFA","Equipment Related","8.46","Very High","","","sensor tested with test gas . audible and visual alarm operation.","2020-01-31","EAGL190006  ","Completed","2020-04-15","No","No","No","Internal","RO currently in  processing stage."]
[null,null,null,null,5168,"38_25/10/2019 6:45:08 PM","2019-07-08","Defect","Ship Staff","Ship Staff Insp.","ME Unit no.3 and unit no 7, Faulty remote exhaust temperature guge.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.21","Medium","","","sensors checked, found defective, same renewed, ","2019-12-31","REAG190222","Completed","2020-02-05","No","No","No","Internal",""]
[null,null,null,null,5246,"38_25/10/2019 8:27:14 PM","2019-07-08","Defect","Ship Staff","Ship Staff Insp.","I.G Deck seal Pp low pressure switch faulty.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.27","Medium","","","Job completed working satisfactory","2019-09-15","REAG190216","Completed","2019-08-21","No","No","No","Internal"]
[null,null,null,null,5253,"38_2019-10-25 20:41:02.000","2019-07-14","Defect","Ship Staff","Ship Staff Insp.","Wind speed indicator in the CCR, high wind speed alarm does not function","Miscellaneous","ISM Related","Equipment Related","5.9","Very High","","","Program Setting corrected and alarms tested , received audioand visual alarm in CCR","2019-08-30","","Completed","2019-08-08","No","No","No","Internal"]
[null,null,null,null,5257,"38_2019-10-25 21:40:31.000","2019-07-14","Defect","Ship Staff","Ship Staff Insp.","M8 mooring winch operating handle leaking","Deck - Mooring Machinery","Mooring","Equipment Related","9.14","Medium","","","Renewed seal, leak arrested, tested ok","2019-07-22","","Completed","2019-07-22","No","No","No","Internal"]
[null,null,null,null,5249,"38_2019-10-25 20:34:36.000","2019-07-20","Defect","Ship Staff","Ship Staff Insp.","Hermetic dip rod wire damaged ( has broken strands), ","Miscellaneous","Cargo / Ballast Systems","Equipment Related","8.12","Medium","","","Renewed MMC DRY CHECK DEVICE  WIRE ROPE.","2019-10-08","REAG 190230","Completed","2019-08-23","No","No","No","Internal"]
[null,null,null,null,5258,"38_2019-10-25 21:43:01.000","2019-07-21","Defect","Ship Staff","Ship Staff Insp.","Forward store port and stbd mushroom vent flaps operation restricted, partially frozen","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","Equipment Related","11.7","High","","","Freed up, lubricated and checked freedom of movement.","2019-07-22","","Completed","2019-07-22","No","No","No","Internal"]
[null,null,null,null,5169,"38_2019-10-25 18:56:36.000","2019-07-30","Defect","Ship Staff","Ship Staff Insp.","PORT PROVISION CRANE HOIST WIRE RUNNER LIMITER FOR BLOCK PROTECTION NON FUNCTIONAL.","Deck - Machinery","Cargo / Ballast Systems","Equipment Related","9.3","Very High","","","Fault Rectified","2020-01-31","","Completed","2019-09-11","No","No","No","Internal","You have indicated in your September 30th DDR that the defect was under investigation and we requested you to revert with findings based on your investigation but to date still no advice on same. Is the investigation completed? If no, when can we expect your findings on same.\n"]
[null,null,null,null,5170,"38_25/10/2019 6:58:55 PM","2019-07-30","Defect","Ship Staff","Ship Staff Insp.","Hyd box no 3, valve CO619 pipe leak from box penetration","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","11.4","Very High","","","Repaired with soft repairs, as this is a penertating pipe Refman raised for Dry Dock repairs.","2020-01-31","","Completed","2019-12-20","No","No","No","Internal","Tech Supt. pls concur transfer of defect to Dry-dock repairs.  \n"]
[null,null,null,null,7764,"38_Fri Oct 25 2019 18:56:36 GMT+0000 (Coordinated Universal Time)","2019-07-30","Defect","Ship Staff","Ship Staff Insp.","PORT PROVISION CRANE HOIST WIRE RUNNER LIMITER FOR BLOCK PROTECTION NON FUNCTIONAL.","Deck - Machinery","Cargo / Ballast Systems","Equipment Related","9.3","Very High","","","Fault rectified","2019-12-31","","Completed","2019-09-11","No","No","No","Internal"]
[null,null,null,null,5212,"38_2019-10-25 19:10:33.000","2019-07-30","Defect","Ship Staff","Ship Staff Insp.","Mooring winches operating lever leaks from MW7. MW5. WL1(port)","Deck - Machinery","Mooring","Equipment Related","9.14","Medium","","","Job completed seals changed tried out founf satisfactory no leaks ","2019-09-30","","Completed","2019-09-18","No","No","No","Internal"]
[null,null,null,null,5239,"38_2019-10-25 20:04:11.000","2019-07-30","Defect","Ship Staff","Ship Staff Insp.","Pump room davit wire, at the hook end has been handle splice","Deck - Machinery","Cargo / Ballast Systems","Equipment Related","5.2","Very High","","","Renewe wire with new spare received vide requisition REAG190243.","2019-09-15","REAG190243","Completed","2019-08-31","No","No","No","Internal"]
[null,null,null,null,5247,"38_2019-10-25 20:28:37.000","2019-07-30","Defect","Ship Staff","Ship Staff Insp.","Draft gauge fwd, aft, mid port have errors exceedin 50 cm","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.5","Very High","","","Blow throught and cleaning done, Visual compared match","2019-08-30","","Completed","2019-08-09","No","No","No","Internal"]
[null,null,null,null,5248,"38_2019-10-25 20:32:03.000","2019-07-30","Defect","Ship Staff","Ship Staff Insp.","Stbd lifeboat aft gripe strands damaged","Miscellaneous","Safety / LSA / FFA","Equipment Related","5.28","Very High","","","Renewed with new gripes rcvd 17 aug 2019","2019-08-30","REAG 190229","Completed","2019-08-23","No","No","No","Internal"]
[null,null,null,null,5171,"38_2019-10-25 19:00:36.000","2019-08-01","Defect","Ship Staff","Ship Staff Insp.","WB edcutor earlier repairs reopened and breached on the discharge side, temporary covered with soft repairs.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.12","Medium","","","Water ballast eductor removed and shifted to E/R workshop. Soft patch section cut and insert put in place. after welding, leak test carried out up to 5.0 bars, no leaks observed. Eductor fitted back and tried out with ballast pump for 30 mins. No leaks observed","2020-02-29","EAGL190061","Completed","2020-02-27","No","No","No","Internal","approved ,awaiting readiness"]
[null,null,null,null,7765,"38_Fri Oct 25 2019 19:00:35 GMT+0000 (Coordinated Universal Time)","2019-08-01","Defect","Ship Staff","Ship Staff Insp.","WB edcutor earlier repairs reopened and breached on the discharge side, temporary covered with soft repairs.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.12","Medium","","","Water ballast eductor removed and shifted to e/r workshop. Hot work carried out and insert fitted. Eductor fitted back after leak test.","2020-01-31","EAGL190061","Completed","2020-02-21","No","No","No","Internal"]
[null,null,null,null,5172,"38_25/10/2019 7:02:42 PM","2019-08-16","Defect","Ship Staff","Ship Staff Insp.","FGDS Pump room O2 sensor defective, does not function","LSA / FFA","Cargo / Ballast Systems","Equipment Related","8.46","Very High","","","Inspection and testing of FGDS done. sensor activated from pumproom. Sensor working satisfactory, audible/visual alarm operational.","2020-01-31","EAGL190006","Completed","2020-04-15","No","No","No","Internal","awaiting readiness"]
[null,null,null,null,5173,"38_25/10/2019 7:04:33 PM","2019-08-16","Defect","Ship Staff","Ship Staff Insp.","FGDS H2S sensor life 24 months, HC sensor 36 months, O2 sensor 24 monrths, no record of when last installed, no spare on board","LSA / FFA","Cargo / Ballast Systems","Equipment Related","8.46","Very High","","","Vessel receiced two O2 sensor in December which was renewed. Testing of gas detection system done. O2 and H2S sensor working fine. Audible and visual alarm activated.","2020-01-31","EAGL190006","Completed","2020-04-15","No","No","No","Internal","After consultation with Tech. Supt, RO for the required spares was submitted and is currently in processing stage."]
[null,null,null,null,5208,"38_25/10/2019 7:04:35 PM","2019-08-16","Defect","Ship Staff","Ship Staff Insp.","Suspected WBT 1s  BA 503 not opening fully","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.18","High","","","Investigated and found the valve inoperational, Removed and found the valve disc in the opposite direction and rubberlining was oversize. The same were corrected and rubber lining renewed. Refitted and tested operation found satisfactory. Pressure tested and no leaks were observed. Checked inside the tank visually working satisfactory.","2019-09-30","","Completed","2019-09-27","No","No","No","Internal"]
[null,null,null,null,5209,"38_25/10/2019 7:05:54 PM","2019-08-16","Defect","Ship Staff","Ship Staff Insp.","Suspected WBT 1s valve/s not holding, BA 503, BA 505","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.18","High","","","Investigated and found the valve inoperational, Removed and found the valve disc in the opposite direction and rubberlining was oversize. The same were corrected and rubber lining renewed. Refitted and tested operation found satisfactory. Pressure tested and no leaks were observed. Checked inside the tank visually working satisfactory.","2019-09-30","","Completed","2019-09-25","No","No","No","Internal"]
[null,null,null,null,5216,"38_2019-10-25 19:18:03.000","2019-08-17","Defect","Ship Staff","Ship Staff Insp.","Port Life Boat, Gear oil leak from winch shaft seal","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.29","High","","","Lowered and checked the winch for leak, no leak found of late, to be observed further.","2019-09-30","","Completed","2019-09-14","No","No","No","Internal"]
[null,null,null,null,5217,"38_25/10/2019 7:19:42 PM","2019-08-17","Defect","Ship Staff","Ship Staff Insp.","Suspect slop S Stripper valve not holding valve no CO 548, slop p CO 542","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.18","High","","","Removed from loaction and found seat intact, with sludge accumilation, cleaned and refitted, tested after fitting in place.","2019-09-30","","Completed","2019-09-09","No","No","No","Internal"]
[null,null,null,null,5231,"38_2019-10-25 19:39:33.000","2019-08-19","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Steering Gear: Minor hydraulic oil leakage from pressure gauge connection on forward starboard side ram.  ","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","leak to rectify by shutting the valve ","2019-08-31","","Completed","2019-08-26","No","No","No","Internal"]
[null,null,null,null,5232,"38_2019-10-25 19:41:06.000","2019-08-19","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","One stanchion in ER on 2nd Deck was found broken.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Stanchion to be welded and put back ","2019-08-31","","Completed","2019-08-26","No","No","No","Internal"]
[null,null,null,null,5237,"38_2019-10-25 19:51:43.999","2019-08-19","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Fire doors: To check all fire doors & adjust hydraulic door closers, to ensure that fire doors remain shut.","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.35","Medium","","","All fire door were adjusted and checked to ensure they remain shut.","2019-08-25","","Completed","2019-08-20","No","No","No","Internal"]
[null,null,null,null,5202,"38_25/10/2019 6:53:17 PM","2019-08-21","Defect","Ship Staff","Ship Staff Insp.","Sewage dosing pump not in operation as defective ","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Dosing pump installed with newly fabricated dosing tank tried put working satisfactory.","2019-10-30","","Completed","2019-10-07","No","No","No","Internal"]
[null,null,null,null,5200,"38_25/10/2019 6:49:45 PM","2019-08-28","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Main cargo steam v/v gasket leaking, to check the gasket size beforehand with correct type of gasket (metal reinforced type) & plan the job during anchorage with boiler shut down.","Cargo Mach.,E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Job completed gasket changed on both side of the valve with metaflex.","2019-10-30","","Completed","2019-10-08","No","No","No","Internal"]
[null,null,null,null,5201,"38_25/10/2019 6:51:29 PM","2019-08-28","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Aircon compressors Amp meter are not showing any reading, same to be checked.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Old ampmeter and current transformer changed with newly recieved spare tried out now working satisfactory.","2019-10-30","","Completed","2019-10-14","No","No","No","Internal"]
[null,null,null,null,5205,"38_25/10/2019 6:58:56 PM","2019-08-28","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","1 port WBT wrong light indication, always showing shut/open both light, same to rectify.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.18","High","","","BA 504 indication error retified by calibrating the valve indicator","2019-10-30","EAGL190033","Completed","2019-09-19","No","No","No","Internal"]
[null,null,null,null,5207,"38_25/10/2019 7:03:16 PM","2019-08-28","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Bilge primary tank heating coil pipe fitting job to be completed","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Job completed ","2019-09-30","","Completed","2019-09-24","No","No","No","Internal"]
[null,null,null,null,5227,"38_2019-10-25 19:34:06.000","2019-08-28","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Sewage plant to be opened & chamber to clean during sailing, transparent hoses to be changed with new ones as no flow is visible from them.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Job to be carried out in open sea ","2019-09-30","","Completed","2019-09-11","No","No","No","Internal"]
[null,null,null,null,5228,"38_2019-10-25 19:35:23.000","2019-08-28","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Slight leaks are observed from Port side steering solenoid v/v & other fitting, same to be cleaned & leakage to be arrested.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Job to be carried out during anchorage ","2019-09-30","","Completed","2019-09-10","No","No","No","Internal"]
[null,null,null,null,5233,"38_2019-10-25 19:42:27.999","2019-08-28","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Lube oil purifier heater steam controller to make operational after fitting the temp sensor pocket into the inlet pipeline.","E/R - Purifier","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Job to be carried out during sailing by stoping purifier.","2019-09-30","","Completed","2019-09-10","No","No","No","Internal"]
[null,null,null,null,5238,"38_2019-10-25 19:54:35.000","2019-08-28","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Fwd air dryer compressor not working, same to be checked.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Job completed","2019-08-30","","Completed","2019-08-29","No","No","No","Internal"]
[null,null,null,null,null,"38_2019-10-25 19:10:48.000","2019-08-28","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","At several location on Main Deck especially near break of accommodation the paint is peeling off and cracked. Same to be grit blasted and recoated after buffing.","Hull & Tanks","General Appearance","External Factors",11.1,"High","Not Applicable","Not Applicable","Peeled off paint being buffed and two coats of paint being applied over affected areas.","2020-01-31",null,"Completed","2020-01-31","No",null,null,"Internal"]
[null,null,null,null,5206,"38_25/10/2019 7:01:26 PM","2019-08-30","Defect","Ship Staff","Ship Staff Insp.","Main IGS pipe aft drain branch pipe leaks at the weld.","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","External Factors","11.4","Very High","","","Repairs done with soft repairs, Leak arrested, Refman to be raised","2019-10-30","","Completed","2019-09-15","No","No","No","Internal"]
[null,null,null,null,5215,"38_25/10/2019 7:16:35 PM","2019-08-30","Defect","Ship Staff","Ship Staff Insp.","Port accommodation ladder pneumatic pipe minor leak","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","Equipment Related","5.47","Medium","","","Renewed pipe with new fabrication","2019-09-30","EAGL195015","Completed","2019-09-05","No","No","No","Internal"]
[null,null,null,null,5213,"38_25/10/2019 7:11:55 PM","2019-09-01","Defect","Ship Staff","Ship Staff Insp.","4 EEBD LEAKING CONTINUOUSLY.","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.44","High","","","SAFETY DISC RECIVED . 4 OF THE EEBD SAFETY DISC CHANGED.","2019-10-09","","Completed","2019-09-10","No","No","No","Internal"]
[null,null,null,null,5220,"38_25/10/2019 7:24:14 PM","2019-09-01","Defect","Ship Staff","Ship Staff Insp.","Fresh water hydrophore pump no.1 discharge valve found not holding valve to be changed.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Fresh water hydrophore pump no.1 discharge valve renewed with overhauled spare as it was passing.","2019-09-20","","Completed","2019-09-12","No","No","No","Internal"]
[null,null,null,null,5224,"38_25/10/2019 7:29:58 PM","2019-09-01","Defect","Ship Staff","Ship Staff Insp.","Aux Boiler no 1  Aux feed water controller malfunction ,same to be rectify","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","overhaul the controller with calibration of SIPART","2019-09-20","","Completed","2019-09-13","No","No","No","Internal"]
[null,null,null,null,5180,"38_25/10/2019 7:18:00 PM","2019-09-03","Defect","Ship Staff","Ship Staff Insp.","Window wiper stbd side some times not working.","Elect. Mach. & Equip.","Navigation","Equipment Related","12.1","High","","","Wiper blade inspected and found in satisfactory condition","2020-01-31","EAGL190034","Completed","2020-03-20","No","No","No","Internal","RFQ approved ,awaiting readiness"]
[null,null,null,null,5204,"38_25/10/2019 6:56:50 PM","2019-09-03","Defect","Ship Staff","Ship Staff Insp.","Suspect FPT valve BA 501 not holding ","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.18","High","","","Investigated and found in good order","2019-10-30","","Completed","2019-09-30","No","No","No","Internal"]
[null,null,null,null,5222,"38_25/10/2019 7:26:56 PM","2019-09-03","Defect","Ship Staff","Ship Staff Insp.","CENTER WINDOW WIPER ONE BLADE NOT WORKING ","Elect. Mach. & Equip.","Navigation","Equipment Related","12.1","High","","","CHECKED FOUND CONNECTION ROD DISSCONNECT AND BELT ALSO DAMAGED SAME RENEWD WITH NEW ONE.","2019-09-05","","Completed","2019-09-05","No","No","No","Internal"]
[null,null,null,null,5179,"38_25/10/2019 7:20:06 PM","2019-09-05","Defect","Ship Staff","Ship Staff Insp.","Steering gear STBD side motor Cooling fan blades found broken","Elect. Mach. & Equip.","Navigation","Equipment Related","10.39","High","","","spares recd at Fujairah on 21 dec 2019","2019-12-27","EAGL190027","Completed","2019-12-23","No","No","No","Internal","spares already provided in Fujairah, close the defect once rectified,"]
[null,null,null,null,5214,"38_25/10/2019 7:13:26 PM","2019-09-05","Defect","Ship Staff","Ship Staff Insp.","1 SCBA SET FOUND LEAKING FROM PRESSURE GAUGE.","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.43","High","","","Pressure gauge link O Ring Changed. No Leak Found","2019-09-30","","Completed","2019-09-06","No","No","No","Internal"]
[null,null,null,null,5223,"38_25/10/2019 7:28:40 PM","2019-09-07","Defect","Ship Staff","Ship Staff Insp.","NO 1 cam shaft lub oil pump found tripping on overload.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","pump dismentaled found rags in the housing ,mechanical seal and bearing renwed.","2019-09-07","","Completed","2019-09-08","No","No","No","Internal"]
[null,null,null,null,5211,"38_2019-10-25 19:08:52.000","2019-09-09","Defect","Ship Staff","Ship Staff Insp.","Alpha lubrication giving alarm for angle deviation.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Adjusted angle encorder according to cylinder 1 TDC","2019-09-25","","Completed","2019-09-21","No","No","No","Internal"]
[null,null,null,null,5221,"38_2019-10-25 19:25:35.000","2019-09-10","Defect","Ship Staff","Ship Staff Insp.","AE#2 unit #1 fuel pump roller found chipped off at the edge.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","AE#2 unit #1 fuel pump roller renewed as the old one was chipped off from the edge","2019-09-10","","Completed","2019-09-10","No","No","No","Internal"]
[null,null,null,null,5199,"38_25/10/2019 6:47:14 PM","2019-09-30","Defect","Ship Staff","Ship Staff Insp.","Port Life boat gear oil leaks from winch shaft","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.29","High","","","Oil level reduced in sump tank. No oil leakage observed thereafter.","2019-10-30","","Completed","2019-10-10","No","No","No","Internal"]
[null,null,null,null,5186,"38_24/10/2019 2:53:19 PM","2019-10-01","Defect","Ship Staff","Ship Staff Insp.","Main FO Flow meter giving erratic reading, AE inlet side Flow meter not operating.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Opened up Flow meter, cleaned all inside, Eased up gears. No Dirt Found, Inlet filter found chocked, same cleaned. ","2019-10-30","","Completed","2019-10-02","No","No","No","Internal"]
[null,null,null,null,7768,"38_Fri Nov 22 2019 11:29:34 GMT+0000 (Coordinated Universal Time)","2019-11-01","Defect","Ship Staff","Ship Staff Insp.","Leakage in hydraulic system detected. Major loss of oil 600 ltrs observed during voy 1905 loading at Mina al Ahmadi. ","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.11","Medium","","","5C COT WASHING & GAS FREED, TOTAL FOUR HYD LINE LEAKAGES RECTIFIED. NO OIL LOSS OBSERVED IN BASRAH LOADING VOY 1907 ","2019-12-31","","Completed","2019-12-20","No","No","No","Internal"]
[null,null,null,null,7770,"38_13/12/2019 5:43:17 PM","2019-11-22","Breakdown","Ship Staff","Ship Staff Insp.","Ecnomiser Feed pump change over pressure switch faulty.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","1.2","Low","","","Defective pressure switch replaced with new spare. fault rectified.","2019-12-30","EAGL190077","Completed","2019-12-24","No","No","No","Internal","vessel has already received spares, update once job is completed"]
[null,null,null,null,7773,"38_15/12/2019 13:54:12","2019-12-03","Non Conformity","Ship Staff","Ship Staff Insp.","DGPS #1 not working properly.","Elect. Mach. & Equip.","Communication","Equipment Related","9.4","High","","","GPS working after shore technician attendance at Fujairah.","2019-12-30","","Completed","2019-12-21","No","No","No","Internal"]
[null,null,null,null,7769,"38_Wed Jun 12 2019 13:34:49 GMT+0000 (Coordinated Universal Time)","2019-12-05","Critical Equipment","Ship Staff","Ship Staff Insp.","Magnetic Compass DC dimmer switch Malfunction.","Elect. Mach. & Equip.","Navigation","Equipment Related","4.2","Medium","","","defective dimmer replaced with new spare","2019-12-20","EAGL190098","Completed","2020-01-13","No","No","No","Internal","RFQ is approved, 3 weeks delivery time,will be connected once ready"]
[null,null,null,null,7774,"38_Sun Dec 15 2019 21:01:25 GMT+0000 (Coordinated Universal Time)","2019-12-05","Non Conformity","Ship Staff","Ship Staff Insp.","ECHO SOUNDER SLEF CHECK SHOWED - S_RAM =NG","Navigation - Echo Sounder / Speed Log","Navigation","Equipment Related","","","","","PCB renewed","2019-12-31","","Completed","2020-01-13","No","No","No","Internal","please take assistance from navsupport"]
[null,null,null,null,7776,"38_Sun Dec 15 2019 21:13:36 GMT+0000 (Coordinated Universal Time)","2019-12-05","Defect","Ship Staff","Ship Staff Insp.","The VDR has been andomly showing an error stating \"Capsule No Connection\" Code 900","Navigation - VDR / BNWAS","Navigation","Equipment Related","","","","","Investigation and checks in progress. Technical Dept. informed.","2020-01-31","EAGL205011 - VDR upgrading from M4 to S1.","Completed","2020-01-30","No","No","No","Internal","VDR upgraded with new model"]
[null,null,null,null,7777,"38_Sun Dec 15 2019 21:25:43 GMT+0000 (Coordinated Universal Time)","2019-12-07","Defect","Ship Staff","Ship Staff Insp.","PORT & STBD LIFEBOAT RUBBER PACKING NOT HOLDING. WATER IS COMING INSIDE.","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.29","High","","","Packing renewed for both port and stbd lifeboat entry doors","2020-01-07","EAGL190104","Completed","2020-01-01","No","No","No","Internal"]
[null,null,null,null,7778,"38_Sun Dec 15 2019 21:28:18 GMT+0000 (Coordinated Universal Time)","2019-12-07","Defect","Ship Staff","Ship Staff Insp.","PORT SIDE LIFEBOAT AIR BOTTLE FILLING CONNECTION LEAKING.","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.29","High","","","Leak rectified.","2020-01-07","","Completed","2019-12-18","No","No","No","Internal"]
[null,null,null,null,7779,"38_Sun Dec 15 2019 22:12:34 GMT+0000 (Coordinated Universal Time)","2019-12-07","Defect","Ship Staff","Ship Staff Insp.","FIRE DOOR PACKING NOT IN GOOD CONDITION","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.35","Medium","","","Fire door packing of C-deck and AC room renewed.","2020-01-30","","Completed","2020-03-28","No","No","No","Internal","spares already supplied last call Fujairah, please close the defect after rectification."]
[null,null,null,null,7780,"38_Sun Dec 15 2019 22:15:04 GMT+0000 (Coordinated Universal Time)","2019-12-07","Defect","Ship Staff","Ship Staff Insp.","BRIDGE PYROTECHNICS ARE 8 AS PER SOLAS SHOOULD BE 12","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.31","High","","","New Pyroctechniques rcvd","2019-12-22","EAGL190099","Completed","2019-12-21","No","No","No","Internal"]
[null,null,null,null,7796,"38_15/12/2019 10:33:47","2019-12-07","Defect","Ship Staff","Ship Staff Insp.","During routine checks on AUS found discharge valve does not follow separator level for all 3 COPT. On putting manual position of AUS and separator level simulation carried out, and found Discharge valve doesnot open corresponding to separator level. ","Cargo Mach.","Cargo / Ballast Systems","Equipment Related,Knowledge Based","","","","","Separator level transmitter calibration carried out for all 3 COPT. AUS calibration carried out for all 3 COPTs and simulation checks carried out , found in good order.","2019-12-31","","Completed","2019-12-11","No","No","No","Internal"]
[null,null,null,null,7797,"38_Mon Dec 16 2019 09:03:55 GMT+0000 (Coordinated Universal Time)","2019-12-07","Defect","Ship Staff","Ship Staff Insp.","LIFEBOAT PORT SIDE SWITCH REMOTE BOX HINGES NOT IN GOOD CONDITION (BROKEN)","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.29","High","","","REPAIRED & HAVE PUT IT BACK","2020-01-07","","Completed","2019-12-12","No","No","No","Internal"]
[null,null,null,null,7798,"38_Mon Dec 16 2019 09:07:19 GMT+0000 (Coordinated Universal Time)","2019-12-07","Defect","Ship Staff","Ship Staff Insp.","SCBA BOTTLE REGULATOR V/V MOVEMENT FREED ","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.35","Medium","","","WORKING PROPERLY","2019-12-09","","Completed","2019-12-08","No","No","No","Internal"]
[null,null,null,null,7786,"38_Mon Dec 16 2019 07:51:26 GMT+0000 (Coordinated Universal Time)","2019-12-08","Other","Ship Staff","Ship Staff Insp.","NAVTOR NAVSTATION APPLICATION IS NOT COMPLETING THE PASSAGE PLANNING SEQUENCE.","Navigation - Others","Navigation","Equipment Related","","","","","PROBLEM NOW FIXED","2019-12-31","","Completed","2019-12-22","No","No","No","Internal"]
[null,null,null,null,7781,"38_Sun Dec 15 2019 22:16:23 GMT+0000 (Coordinated Universal Time)","2019-12-09","Defect","Ship Staff","Ship Staff Insp.","EEBD LEAKING ","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.44","High","","","REFILLED AND TESTED. NO LEAK FOUND. MAINTAINING REQUIRED PRESSURE.","2019-12-20","","Completed","2020-01-02","No","No","No","Internal","its almost a month, please advice reason for pending"]
[null,null,null,null,7788,"38_Mon Dec 16 2019 09:17:29 GMT+0000 (Coordinated Universal Time)","2019-12-10","Defect","Ship Staff","Ship Staff Insp.","Pilot ladder not in good condition","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.47","Medium","","","New pilot ladder installed.","2020-01-25","EAGL190038","Completed","2020-01-16","No","No","No","Internal","please raise new RFQ in year 2020"]
[null,null,null,null,7795,"38_15/12/2019 10:19:49","2019-12-10","Defect","Ship Staff","Ship Staff Insp.","IG sampling line gets frequently choke and sampling bubbles reduces after some time and stops.","Inert Gas","Cargo / Ballast Systems","Equipment Related","","","","","Checks carried out on IG sampling and found pressure regulator valve seat corroded and valve in bad shape. Same replaced with new regulator, system tried out found in good order.","2019-12-15","","Completed","2019-12-14","No","No","No","Internal"]
[null,null,null,null,7782,"38_Sun Dec 15 2019 22:24:07 GMT+0000 (Coordinated Universal Time)","2019-12-11","Defect","Ship Staff","Ship Staff Insp.","SI LIGHTS FOR LIFEJACKET & IMMERSION SUIT EXPIRING IN JANUARY 2020","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.31","High","","","NEW SI LIGHTS RECEIVED AT FUJAIRAH. ALL JAN EXPIRED LIGHTS REPLACED DURING MONTHLY INSPECTION. ALL IN ORDER.","2020-01-10","EAGL190074","Completed","2020-01-08","No","No","No","Internal","please advice the RFQ number"]
[null,null,null,null,7771,"38_Sun Dec 15 2019 14:31:42 GMT+0000 (Coordinated Universal Time)","2019-12-12","Non Conformity","Ship Staff","Ship Staff Insp.","Stripping pump strokes indicator does not show strokes in CCR. ","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.8","Medium","","","Stripping pump stroke indicator was inspected, storke converter was not working properly. now all parts cleaned, now showing stroke reading in CCR.","2020-01-20","","Completed","2020-09-15","No","No","No","Internal","please let us know the progress of the job"]
[null,null,null,null,7775,"38_Sun Dec 15 2019 21:06:49 GMT+0000 (Coordinated Universal Time)","2019-12-12","Defect","Ship Staff","Ship Staff Insp.","COURSE RECORDER PRINTING INCORRECT DATE","Navigation - Others","Navigation","Equipment Related","4.7","High","","","Job completed. Procedure for inputting the settings was being wrongly followed.","2019-12-31","","Completed","2020-11-19","No","No","No","Internal","service attendance carried out at fujairah"]
[null,null,null,null,7772,"38_Sun Dec 15 2019 14:34:06 GMT+0000 (Coordinated Universal Time)","2019-12-13","Defect","Ship Staff","Ship Staff Insp.","COP No1 trip not activating from CCR","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.74","High","","","stop solenoid checked, COP trip tried out from all location found working satisfactory","2020-01-31","","Completed","2020-01-03","No","No","No","Internal","keep us updated on troubleshooting progress"]
[null,null,null,null,7783,"38_Mon Dec 16 2019 07:13:16 GMT+0000 (Coordinated Universal Time)","2019-12-15","Defect","Ship Staff","Ship Staff Insp.","BNWAS WAS OBERVED TO MISS 12 mins INTERVAL ALERTS AT TIMES. THIS IS NOT FREQUENT THOUGH. NORMALLY ALERTS THE OOW AT EVERY 12 MINS.","Navigation - VDR / BNWAS","Navigation","Equipment Related","","","","","System found working satisfactory. At present","2019-12-31","","Completed","2020-01-29","No","No","No","Internal","keep us updated on troubleshooting progress"]
[null,null,null,null,7789,"38_Mon Dec 16 2019 10:48:29 GMT+0000 (Coordinated Universal Time)","2019-12-15","Non Conformity","Ship Staff","Ship Staff Insp.","Eight rope tails more than 18 months old. Needs renewal.","Deck - Machinery,Deck - Mooring Machinery","Mooring","Equipment Related","9.5","High","","","New tail ropes rcvd and renewal done","2019-12-31","EAGL195026","Completed","2019-12-21","No","No","No","Internal"]
[null,null,null,null,7790,"38_Mon Dec 16 2019 10:55:11 GMT+0000 (Coordinated Universal Time)","2019-12-15","Defect","Ship Staff","Ship Staff Insp.","Light fittings around accomodation rusted. Shades have become opaque.","Elect. Mach. & Equip.","General Appearance","Equipment Related","11.9","Low","","","De-rusting and hot work over wasted fittings. Renewal of shades of lights Requisition made, awaiting for spares/ all accommodation wasted fittings were changed with new spare fitting.","2020-02-15","EAGL190105 . EAGL200270","Completed","2020-09-09","No","No","No","Internal"]
[null,null,null,null,7791,"38_Mon Dec 16 2019 11:01:16 GMT+0000 (Coordinated Universal Time)","2019-12-15","Defect","Ship Staff","Ship Staff Insp.","Gangway air lines observed rusted. Requires maintenance.","Deck - Machinery","Structural Condn. / WT integrity ","Equipment Related","11.4","Very High","","","Maintenance carried out. Wasted pipelines renewed. Presently no leakages.","2020-02-15","","Completed","2020-11-02","No","No","No","Internal"]
[null,null,null,null,7794,"38_Mon Dec 16 2019 11:28:46 GMT+0000 (Coordinated Universal Time)","2019-12-15","Defect","Ship Staff","Ship Staff Insp.","PORT SIDE LIFEBOAT HAVE CHAFFING ON IT","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.29","High","","","CRACK FILLED AND PAINTED","2020-01-15","","Completed","2020-01-05","No","No","No","Internal"]
[null,null,null,null,7784,"38_Mon Dec 16 2019 07:16:39 GMT+0000 (Coordinated Universal Time)","2019-12-16","Defect","Ship Staff","Ship Staff Insp.","AIS SHOWING ERROR: MKD CONNECTION LOST","Navigation - DGPS / EPFS / AIS","Navigation","Equipment Related","","","","","RF cable found defcetive and same renewed. now equipment working satisfactory.","2019-12-31","","Completed","2020-03-04","No","No","No","Internal","keep us updated on troubleshooting progress"]
[null,null,null,null,7785,"38_Mon Dec 16 2019 07:23:12 GMT+0000 (Coordinated Universal Time)","2019-12-16","Defect","Ship Staff","Ship Staff Insp.","WINDOW WIPER BLADES DAMAGED, DUE FOR REPLACEMENT","Accommodation","General Appearance","Equipment Related","","","","","THE WIPER BLADES REPLACED WITH SPARE WIPER BLADES.","2019-12-31","","Completed","2019-12-23","No","No","No","Internal"]
[null,null,null,null,9374,"38_31-Dec-19 5:43:01 PM","2019-12-19","Defect","Ship Staff","Ship Staff Insp.","SAT-C NO.2  PRINTER ERROR","Navigation - GMDSS & Communication","Navigation","Equipment Related","","","","","NEW PRINTER RECEIVED AT SINGAPORE. INSTALLED","2020-01-15","","Completed","2020-01-12","No","No","No","Internal","please raise RFQ"]
[null,null,null,null,9378,"38_02/01/2020 17:55:27","2019-12-19","Breakdown","Ship Staff","Ship Staff Insp.","On routine round aux engine found giving abnormal noise and vibration. On stopping after inspection found camshaft for unit no. 6 damaged.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Cam shaft for unit no.6 for aux engine #3 was replaced with new spare, along with rollers and roller housing.","2019-12-21","","Completed","2019-12-20","No","No","No","Internal"]
[null,null,null,null,9379,"38_02/01/2020 18:03:55","2019-12-19","Defect,Observation","Ship Staff","Ship Staff Insp.","On routine rounds ship staff noticed a steam leak from valve bonnet of circ pump discharge to boiler.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","Steam line was isolated and valve bonnet gasket replaced with new spare fabricated on board. Steam leak rectified.","2019-12-22","","Completed","2019-12-19","No","No","No","Internal"]
[null,null,null,null,12350,"38_03/01/2020 0:39:23","2019-12-21","Non Conformity","Ship Staff","Ship Staff Insp.","Crew elevator not functional. Technician visited vessel, as per report the EPROM of ENCODER card is malfunctioning.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","shore technician attended the vessel at Fujairah on 11 May 2020. found Eprom card and IC defective same renewed. Elevator working satisfactory","2020-01-15","","Completed","2020-05-11","No","No","No","Internal"]
[null,null,null,null,9381,"38_02/01/2020 19:34:56","2019-12-22","Observation","Ship Staff","Ship Staff Insp.","Incinerator refractory during routine inspection was found to be damaged and in bad shape.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","Incinerator refractory was repaired from bilbrico cement available onboard.","2019-12-30","","Completed","2019-12-22","No","No","No","Internal"]
[null,null,null,null,9375,"38_31-Dec-19 5:46:21 PM","2019-12-23","Defect","Ship Staff","Ship Staff Insp.","COT 5C HIGH HIGH LEVEL ALARM NOT RESETTING AFTER TRYING OUT.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.14","Very High","","","DEFECTIVE FLOAT REPLACED WITH NEW FLOAT. SYSTEM TESTED. WORKING SATISFACTORY.","2020-03-15","","Completed","2020-03-03","No","No","No","Internal","spare approved,awaiting readiness,keep us updated on progress"]
[null,null,null,null,9376,"38_31-Dec-19 5:50:07 PM","2019-12-24","Defect","Ship Staff","Ship Staff Insp.","ODME calibration unsuccesful due to \"EPU Flow2 underrange\", and EPU no skid flow alarms.","Critical Equip.","Cargo / Ballast Systems","Equipment Related","6.13","Low","","","Advice taken from manufacturer. Sample outlet line cleared, alarm reset, calibration successful.","2020-01-15","","Completed","2020-01-12","No","No","No","Internal","troubleshooting send to maker for assistance, to be followed up"]
[null,null,null,null,9377,"38_31-Dec-19 5:52:30 PM","2019-12-24","Defect","Ship Staff","Ship Staff Insp.","Hydraulic Leak Observed from port side midship crane runner winch associated flexible hose.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.5","Very High","","","Two O-rings renewed for hydru, leak rectified","2020-01-15","","Completed","2020-01-10","No","No","No","Internal","Please keep us updated on progress"]
[null,null,null,null,9383,"38_02/01/2020 20:16:14","2019-12-24","Defect","Ship Staff","Ship Staff Insp.","During EBG washing ship staff observed the drain valve to soot collecting tank was stuck in closed positon.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","Valve to the soot collecting from EBG drain was replaced with new spare valve available onboard.","2019-12-31","","Completed","2019-12-24","No","No","No","Internal"]
[null,null,null,null,9380,"38_02/01/2020 18:10:58","2019-12-25","Defect","Ship Staff","Ship Staff Insp.","Main engine unit 2 and 7 indicator cocks found leaking, and 1,3,5and 6 found choked.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","All indicator cocks were taken out and overhauled. checked and found in good working order.","2019-12-30","","Completed","2019-12-27","No","No","No","Internal"]
[null,null,null,null,9382,"38_02/01/2020 20:12:17","2019-12-26","Observation","Ship Staff","Ship Staff Insp.","Lube oil found leaking from Main engine chain case coved.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Lube oil leak rectified from chain cover gasket on putting back up gasket in grove. As the gasket found was not pertuded. leak rectified.","2019-12-31","","Completed","2019-12-26","No","No","No","Internal"]
[null,null,null,null,12300,"38_08/01/2020 12:34:01 PM","2020-01-05","Critical Equipment","Ship Staff","Engineering Audit","Fire and GS Pump no 1 motor terminal lugs burnt","LSA / FFA","Eng. / Strg. Comp.","Equipment Related","","","","","lugs replaced with the spare lugs","2020-01-07","","Completed","2020-01-07","No","No","No","Internal"]
[null,null,null,null,12280,"38_14/01/2020 12:17:18 PM","2020-01-05","Defect","Ship Staff","Ship Staff Insp.","Purifier room entrance fire door (fwd) in poor state, made only from sheet, ","LSA / FFA","Eng. / Strg. Comp.","Equipment Related","","","","","temporary repair carried out. ","2020-01-31","","Completed","2020-06-17","No","No","No","Internal"]
[null,null,null,null,12301,"38_08/01/2020 12:39:12 PM","2020-01-07","Defect","Ship Staff","Engineering Audit","E/R Alarm monitoring system station 1 CPU not rebooting","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","Request has been sent for maker advise ","2020-01-16","","Completed","2020-01-12","No","No","No","Internal"]
[null,null,null,null,12276,"38_08/01/2020 12:42:07 PM","2020-01-07","Defect","Ship Staff","Engineering Audit","Aux Engine no 3 can not put on stand by mode","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Maker advise has been requested. External supply to PLC unit given on 21st july 2020 to activate the safeties. The Luboil pressure switch was renew.","2020-01-15","","Completed","2020-08-13","No","No","No","Internal","service attendance carried out in fujiarah, Suspected parts on order & will be delivered to vessel"]
[null,null,null,null,12277,"38_08/01/2020 2:44:45 PM","2020-01-07","Critical Equipment","Ship Staff","ISM Audit","Deck foam fire fighting system, foam pump mechanical seal leaking","Critical Equip.,LSA / FFA","Emgcy. Systems","Equipment Related","5.35","Medium","","","DECK FOAM PUMP MECHANICAL SEAL WAS RENEWED WITH NEW RECEIVED SPARE SEAL, PUMP TRIED OUT WITH FRESH WATER, NO LEAK OBSERVED.","2020-12-30","EAGL200014","Completed","2020-11-11","No","No","No","Internal"]
[null,null,null,null,12318,"38_10/01/2020 8:37:23 PM","2020-01-10","Defect","Ship Staff","Engineering Audit","440V Low insulation from Galley hot plate","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.38","Medium","","","defective hot plate replaced with new spare","2020-01-20","","Completed","2020-03-10","No","No","No","Internal"]
[null,null,null,null,12283,"38_14/01/2020 4:33:39 PM","2020-01-10","Defect","Ship Staff","Ship Staff Insp.","ICCP panel in ECR not showing any reading","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","To investigate and request for spares if required/ New Aft ICCP full unit was installed earlier, ECR unit is not in use.","2020-01-31","","Completed","2020-08-30","No","No","No","Internal"]
[null,null,null,null,12288,"38_18-Jan-20 2:24:50 PM","2020-01-12","Defect","Ship Staff","Ship Staff Insp.","LSMGO line stbd side manifold heavily rusted.","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","Equipment Related","11.4","Very High","","","pipe section removed. new pipe section fabricated and put in place","2020-02-14","","Completed","2020-06-01","No","No","No","Internal"]
[null,null,null,null,12302,"38_19-Jan-20 8:54:47 AM","2020-01-12","Defect","Ship Staff","Ship Staff Insp.","Mast riser female quick coupling connection for CO2 extinguisher rusty & not usable.","LSA / FFA","Emgcy. Systems","Equipment Related","5.35","Medium","","","Quick coupling to be renewed.","2020-01-31","","Completed","2020-01-16","No","No","No","Internal"]
[null,null,null,null,12322,"38_19-Jan-20 9:03:39 AM","2020-01-12","Observation","Ship Staff","Ship Staff Insp.","Access to fpk str port side bilge restricted due to mooring wires & ropes.","Miscellaneous","General Appearance","Human Error","6.15","High","","","Area to be cleared and clear access made","2020-01-25","","Completed","2020-02-08","No","No","No","Internal"]
[null,null,null,null,12323,"38_19-Jan-20 9:07:24 AM","2020-01-12","Observation","Ship Staff","Ship Staff Insp.","Hydraulic oil drum securing done to sounding pipe in fwd fpk store.","Miscellaneous","General Appearance","Human Error","5.11","Low","","","Drums secured to the strong point","2020-01-31","","Completed","2020-02-07","No","No","No","Internal"]
[null,null,null,null,12324,"38_19-Jan-20 9:12:53 AM","2020-01-12","Observation","Ship Staff","Ship Staff Insp.","No ear defender kept at the entrance of FPK store","Miscellaneous","General Appearance","Human Error","5.5","Low","","","Ear defenders placed at the entrance of FPK store.","2020-01-28","","Completed","2020-02-01","No","No","No","Internal"]
[null,null,null,null,12340,"38_19-Jan-20 8:58:48 AM","2020-01-12","Observation","Ship Staff","Ship Staff Insp.","Insulation mat for fwd ICCP missing","Miscellaneous","Eng. / Strg. Comp.","Human Error","10.24","Low","","","Insulation mat put in place","2020-01-30","","Completed","2020-01-16","No","No","No","Internal"]
[null,null,null,null,12341,"38_18-Jan-20 2:50:07 PM","2020-01-12","Defect","Ship Staff","Ship Staff Insp.","W2A winch hydraulic pipes heavily rusted.","Deck - Mooring Machinery","Mooring","Equipment Related","11.4","Very High","","","Grit blasting & painting carried out.","2020-03-30","","Completed","2020-03-18","No","No","No","Internal"]
[null,null,null,null,12345,"38_19-Jan-20 9:20:20 AM","2020-01-12","Observation","Ship Staff","Ship Staff Insp.","Greasing required for pumproom blowers","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Knowledge Based","5.18","High","","","Greasing carried out.","2020-01-31","","Completed","2020-01-29","No","No","No","Internal"]
[null,null,null,null,12346,"38_18-Jan-20 2:13:59 PM","2020-01-12","Defect","Ship Staff","Ship Staff Insp.","Hydraulic line inlet and outlet support wasted.","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","Equipment Related","11.4","Very High","","","No.2 nd No.3 mooring winch hydraulic linlet and out lines grit blasted and painting carried out.","2020-03-15","","Completed","2020-02-25","No","No","No","Internal"]
[null,null,null,null,12365,"38_18-Jan-20 2:44:46 PM","2020-01-12","Defect","Ship Staff","Suptd. Insp.","Port side midship store light bonding wire missing.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","8.48","Medium","","","Bonding wire fitted","2020-01-31","","Completed","2020-01-30","No","No","No","Internal"]
[null,null,null,null,12366,"38_18-Jan-20 2:47:42 PM","2020-01-12","Observation","Ship Staff","Ship Staff Insp.","Port side cargo crane hose, 2 nos showing aging cracks.","Deck - Machinery","Cargo / Ballast Systems","Equipment Related","8.5","Very High","","","ALL THE HOSES INSPECTED, FOUND ALL IN GOOD CONDITION, NO CRACKS FOUND.","2020-02-15","","Completed","2020-09-21","No","No","No","Internal"]
[null,null,null,null,12367,"38_19-Jan-20 9:16:24 AM","2020-01-12","Observation","Ship Staff","Ship Staff Insp.","Manila rope for pumproom rescue faulty, as it will burn in case of fire","LSA / FFA","Emgcy. Systems","Human Error","5.13","High","","","Fire retardent rope is put in place.","2020-01-31","","Completed","2020-05-29","No","No","No","Internal"]
[null,null,null,null,12286,"38_18-Jan-20 2:16:17 PM","2020-01-12","Defect","Ship Staff","Ship Staff Insp.","Mooring winch 4B pressure relief valve cover wasted","Deck - Mooring Machinery","Mooring","Equipment Related","9.14","Medium","","","Completed","2020-02-15","","Completed","2020-02-15","No","No","No","Internal"]
[null,null,null,null,12287,"38_18-Jan-20 2:20:47 PM","2020-01-12","Defect","Ship Staff","Ship Staff Insp.","Port and stbd gangway air lines, trolley chain, angle support, heavily rusted, wasted. Top sheaves not rotating.","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","Equipment Related","11.4","Very High","","","Trolley wheels freed and greased. Maintenance on Air lines carried out. Sheaves made free and greased.","2020-03-15","","Completed","2020-10-30","No","No","No","Internal"]
[null,null,null,null,null,"38_18-Jan-20 2:06:38 PM","2020-01-12","Defect","Ship Staff","Ship Staff Insp.","Many mooring winch gear hydraulic oil tank gauge glass painted over, have become fully opaque.","Deck - Mooring Machinery","Mooring","Equipment Related",9.14,"Medium","Not Applicable","Not Applicable","The 4pcs sight glass was  renew.","2020-02-12",null,"Completed","2020-12-24","No",null,null,"Internal"]
[null,null,null,null,null,"38_19-Jan-20 9:25:42 AM","2020-01-12","Observation","Ship Staff","Ship Staff Insp.","Pumproom natural vent rubber packing wasted","Deck - Pipe / Fittings","Eng. / Strg. Comp.","Equipment Related",8.44,"High","Not Applicable","Not Applicable","Rubber packing to be renewed","2020-02-15",null,"Completed","2020-12-01","No",null,null,"Internal"]
[null,null,null,null,12303,"38_18-Jan-20 8:40:25 AM","2020-01-13","Defect","Ship Staff","Ship Staff Insp.","Pump room IS sound powered telephone headset non operational. However handset is operational.","Elect. Mach. & Equip.","Communication","Equipment Related","5.17","Very High","","","Repeated observation","2020-02-15","","Completed","2020-01-29","No","No","No","Internal"]
[null,null,null,null,12304,"38_13/01/2020 7:49:15 AM","2020-01-13","Defect","Owner / Marine / Tech. Suptd.","Engineering Audit","Atm condenser end cover (sea water inlet side) has fine seepage marks, suspected metal thinning","E/R - Aux. Mach.,E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","End cover removed and repaired in E/R workshop. put back in place","2020-01-31","","Completed","2020-01-30","No","No","No","Internal"]
[null,null,null,null,12305,"38_13/01/2020 1:45:48 PM","2020-01-13","Defect","Ship Staff","Ship Staff Insp.","ME Jacket cooling water inlet remote temp sensor not working","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","sensor checked, found defective, same renewed","2020-01-20","","Completed","2020-01-13","No","No","No","Internal"]
[null,null,null,null,12316,"38_14/01/2020 4:39:59 PM","2020-01-13","Observation","Ship Staff","Ship Staff Insp.","Emergency generator cooling water line flexible hoses has cracks/wear down marks","E/R - Aux. Mach.","Emgcy. Systems","Equipment Related","","","","","Hoses renewed","2020-01-20","","Completed","2020-03-22","No","No","No","Internal"]
[null,null,null,null,12278,"38_13/01/2020 5:04:50 PM","2020-01-13","Defect","Ship Staff","Ship Staff Insp.","Aux Boiler (port side ) water level increasing when preheat steam is opened","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.38","Medium","","","internal inspection of the boiler water side carried out, found no leaks","2020-01-31","","Completed","2020-04-05","No","No","No","Internal","coil pressure tested & Found satisfactory, controller overhauled"]
[null,null,null,null,12279,"38_13/01/2020 5:11:53 PM","2020-01-13","Breakdown,Defect","Ship Staff","Ship Staff Insp.","HFO Purifier no 1, horozontal shaft worm gear found worn out","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","complete overhaul carried out, purifier tried out, found working satisfactory","2020-01-15","","Completed","2020-03-05","No","No","No","Internal"]
[null,null,null,null,12312,"38_14/01/2020 12:23:13 PM","2020-01-14","Defect","Ship Staff","Ship Staff Insp.","COPT Platform telephone 1 button not working","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","5.17","Very High","","","spares received, defective key pad replaced with new spare","2020-01-31","","Completed","2020-03-21","No","No","No","Internal"]
[null,null,null,null,12313,"38_14/01/2020 12:20:11 PM","2020-01-14","Defect","Ship Staff","Ship Staff Insp.","Telephone near ME local manouvering found 1 button not working, ","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","5.17","Very High","","","defective key pad replaced with new spare","2020-01-31","","Completed","2020-03-21","No","No","No","Internal"]
[null,null,null,null,12317,"38_14/01/2020 1:20:45 PM","2020-01-14","Critical Equipment","Ship Staff","Ship Staff Insp.","Incinerator Low vac in combustion chamber alarm not working, Atm air low pressure alarm not working","Critical Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","defective part replaced with new spare","2020-01-20","","Completed","2020-02-05","No","No","No","Internal"]
[null,null,null,null,12281,"38_14/01/2020 12:25:56 PM","2020-01-14","Defect","Ship Staff","Ship Staff Insp.","Pump room bottom platform telephone headset not working","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","5.17","Very High","","","new telephone received and installed. tested , working satisfactory","2020-01-31","","Completed","2020-06-14","No","No","No","Internal","spares had lead time for readiness ,will be supplied to vessel on 13th june20"]
[null,null,null,null,12311,"38_14/01/2020 5:17:55 PM","2020-01-15","Observation","Ship Staff","Ship Staff Insp.","Fire detector at C deck infront of ETO cabin found taped at the head. ","LSA / FFA","Eng. / Strg. Comp.","Equipment Related","","","","","tape removed, detector tried out, found working satisfactory","2020-01-20","","Completed","2020-01-19","No","No","No","Internal"]
[null,null,null,null,12315,"38_15/01/2020 5:29:31 AM","2020-01-15","Defect","Ship Staff","Ship Staff Insp.","No lubrication for #5 unit exhaust valve rocker arn on AE #3.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Rocker arm removed and checked for any damages. All holes blown with compressed air and found clear. Found that the Bush on the rocker arm shifting position during running condition. Requires replacement because of the lifetime.Manual lubrication to be carried out using portable hand oil pump and contionous monitioring of the particular unit during running condition.Bush replaced with new spares","2020-01-31","EAGL190072","Completed","2020-01-28","No","No","No","Internal"]
[null,null,null,null,12368,"38_27-Jan-20 1:34:48 PM","2020-01-24","Defect","Ship Staff","Ship Staff Insp.","One out of three valve hydraulic hand pump hose damaged.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","New Hose received & renewal.","2020-02-15","EAGL200052","Completed","2020-08-24","No","No","No","Internal"]
[null,null,null,null,12328,"38_03-Mar-20 10:07:01 AM","2020-02-02","Defect","Ship Staff","Ship Staff Insp.","APk tank remote sounding guage inoperational.","Hull & Tanks","Cargo / Ballast Systems","Equipment Related","","","","","Remote sounding pipe found heavily choked. Tried to clear by hammering/Air blow/chemicals without any success. Finally pipe cut from about 2.0m above bottom as bottom is inaccessible due to extreme narrow openings. Permanent repairs to be done during next docking.","2020-03-31","","Completed","2020-03-25","No","No","No","Internal"]
[null,null,null,null,12360,"38_03-Mar-20 9:20:07 AM","2020-02-02","Defect","Ship Staff","Ship Staff Insp.","FPK TANK VALVE BA 501 LEAKING. ","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","new valve received at fujairah on 08.05.2020. Valve renewed and tested. Found working with no leaks","2020-05-30","","Completed","2020-05-21","No","No","No","Internal"]
[null,null,null,null,12362,"38_03-Mar-20 10:05:06 AM","2020-02-02","Defect","Ship Staff","Ship Staff Insp.","FPK tank remote sounding gauge inoperational.","Hull & Tanks","Cargo / Ballast Systems","Equipment Related","","","","","same job raised in Aug-2019 as ballast draft gauge malfunction.","2020-03-31","","Completed","2020-11-17","No","No","No","Internal"]
[null,null,null,null,12319,"38_03-Mar-20 10:30:26 AM","2020-02-06","Defect","Ship Staff","Ship Staff Insp.","WBT 5S tank dome butterfly nut hinge wasted/broken","Hull & Tanks","Structural Condn. / WT integrity ","Equipment Related","","","","","New lug welded for butterfly nut. Hot work carried out after obtaining office permission","2020-03-31","","Completed","2020-03-27","No","No","No","Internal"]
[null,null,null,null,12291,"38_26/02/2020 11:34:51 AM","2020-02-08","Defect","Ship Staff","Ship Staff Insp.","ECR VOIP phone incoming ring tone not audible","Miscellaneous","Communication","Equipment Related","","","","","Confirm ECR VOIP phone working good condition .","2020-04-10","","Completed","2020-11-17","No","No","No","Internal","checked & communicated, working satisfactory"]
[null,null,null,null,12339,"38_03-Mar-20 9:39:18 AM","2020-02-08","Defect","Ship Staff","Ship Staff Insp.","During load test prior arrival load port, it was observed that Stbd hose handling crane not holding weight more than 5.6 T and luffing wire drum is slipping.","Deck - Machinery","Cargo / Ballast Systems","Equipment Related","","","","","Counter balance valve seals found damaged. New seals receibed in singapore and same renewed. Crane operted and load tested to 18.3 tonnes and found holding weight. Working satisfactory.","2020-04-30","","Completed","2020-04-19","No","No","No","Internal"]
[null,null,null,null,12330,"38_03-Mar-20 9:43:30 AM","2020-02-10","Defect","Ship Staff","Ship Staff Insp.","During 3 monthly lowering and manoeuvering drill it was observed that Stbd life boat coxwain hatch is leaking during sprinkler test.","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","Rubber packing of the coxwain hatch replaced with new one","2020-02-29","","Completed","2020-03-16","No","No","No","Internal"]
[null,null,null,null,12336,"38_03-Mar-20 9:49:08 AM","2020-02-10","Defect","Ship Staff","Ship Staff Insp.","POrt side lifeboat 3 seat belts lock are defective.","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","New seat belts received at Khorfakkan and fitted.","2020-03-31","","Completed","2020-04-09","No","No","No","Internal"]
[null,null,null,null,12349,"38_03-Mar-20 9:45:26 AM","2020-02-10","Defect","Ship Staff","Ship Staff Insp.","During 3 monthly lifeboat lowering and manoeuvering drill it was observed that stbd lifeboat shaft seal is leaking water","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","To be inspected and seal or gland packing to be renewed. On close inspection found sprinkler pump casing damaged, pump replaced with new spare pump ","2020-02-29","","Completed","2020-05-09","No","No","No","Internal"]
[null,null,null,null,12293,"38_04-Mar-20 12:54:07 PM","2020-02-11","Defect","Ship Staff","Ship Staff Insp.","echo sounder showing “SRam : NG” Error and failure of self check.","Navigation - Echo Sounder / Speed Log","Navigation","Equipment Related","","","","","vessel received new PCB for the echo sounder “SRam : NG” error was rectified. Upon self diagnosis, all checks were coming OK. but with new PCB it was observed no depth readings shown and showing “Bottom lost” error. hence unable to show depth.  OLC pcb put back. Vessel awaiting for office advice. - Under Observation, presently there is no alarm.","2020-03-31","","Completed","2020-11-10","No","No","No","Internal","new PCB fitted & rectified"]
[null,null,null,null,12310,"38_03-Mar-20 10:39:47 AM","2020-02-17","Defect","Ship Staff","Ship Staff Insp.","One of the supper drain pipe found holed located in China passage area leading from A-deck to Upper deck","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","Equipment Related","","","","","Weld filling carried out of the scupper drain pipe by carrying out hot work after abtaining office approval.","2020-03-31","","Completed","2020-03-17","No","No","No","Internal"]
[null,null,null,null,12344,"38_03-Mar-20 10:36:43 AM","2020-02-19","Defect","Ship Staff","Ship Staff Insp.","Fixed gas detection system for WBT tested during FPK tank inspection by locally applying test gas. No alarm detected in the panel. Later on system tripped showing \"No vaccum detected\"","Elect. Mach. & Equip.","Cargo / Ballast Systems","Equipment Related","","","","","Solonoid switches found dirty. Solonoid cleaned and fitted back by ETO. System tested with test gas from WBT 3S and WBT 5P. Alarm received in CCR. Other tanks also to be tested during tank entry.","2020-03-31","","Completed","2020-04-12","No","No","No","Internal"]
[null,null,null,null,12307,"38_26/02/2020 12:04:08 PM","2020-02-20","Defect","Ship Staff","Ship Staff Insp.","Bilge holding tank high level alarm not working","Hull & Tanks","Eng. / Strg. Comp.","Equipment Related","","","","","Float lever found broken, float renewed. alarm tested found working satisfactory","2020-02-23","","Completed","2020-02-23","No","No","No","Internal"]
[null,null,null,null,12314,"38_22/02/2020 12:06:50 PM","2020-02-21","Breakdown,Defect,Observation","Ship Staff","Ship Staff Insp.","Bilge holding tank high level alarm found not working","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","Float found damaged, same replaced with new spare . Alarm tested found working satisfactory","2020-02-24","","Completed","2020-02-22","No","No","No","Internal"]
[null,null,null,null,12308,"38_26/02/2020 12:07:19 PM","2020-02-23","Defect","Ship Staff","Ship Staff Insp.","SBOT tank high level alarm found not working","Hull & Tanks","Eng. / Strg. Comp.","Equipment Related","","","","","Float found defective same replaced with new spare","2020-02-26","","Completed","2020-02-26","No","No","No","Internal"]
[null,null,null,null,12306,"38_26/02/2020 12:00:40 PM","2020-02-24","Defect","Ship Staff","Ship Staff Insp.","ME Lub oil sump low level alarm found not working","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Float check, adjustment carried out, found working satisfactory","2020-02-26","","Completed","2020-02-26","No","No","No","Internal"]
[null,null,null,null,12320,"38_03-Mar-20 10:12:06 AM","2020-02-25","Defect","Ship Staff","Ship Staff Insp.","One of the hinge of the Port sidelight cover broken","Miscellaneous","Structural Condn. / WT integrity ","Equipment Related","","","","","Hot work completed after obtaining hot work approval from office","2020-03-31","","Completed","2020-03-14","No","No","No","Internal"]
[null,null,null,null,12321,"38_03-Mar-20 10:08:43 AM","2020-02-25","Defect","Ship Staff","Ship Staff Insp.","Apk sounding pipe chocked","Hull & Tanks","Cargo / Ballast Systems","Equipment Related","","","","","Sounding found choked from bottom, Tank bottom inaccessible due to unavailibility of manholes and extremely confined openings. Tried to clear sounding pipe by hammering/Air blowing/Chemicals without any success. Hole made in sounding pipe at about 2.0 above bottom for water access. Work to be undertaken during dry dock for permanent repairs","2020-03-31","","Completed","2020-03-25","No","No","No","Internal"]
[null,null,null,null,12292,"38_04-Mar-20 12:44:40 PM","2020-02-27","Defect","Ship Staff","Ship Staff Insp.","while trying to record data in data recording software connected to bridge PC Communication Error Pop’s up and unable to record the data.","Navigation - Echo Sounder / Speed Log","Navigation","Equipment Related","","","","","Serial port settings for the communication from the PC to Echosounder was changed from COM2 to COM1 and it was rectified. Now Echosounder data could be recorded on  Bridge PC like Normal.","2020-03-31","","Completed","2020-10-21","No","No","No","Internal","communication between service provider & vessel in progress to find root cuase"]
[null,null,null,null,12325,"38_03/04/2020 9:54:58 AM","2020-03-03","Defect","Ship Staff","Ship Staff Insp.","Main cooling sea water pump no1 inlet pipe sectionfound leaking","E/R - Aux. Mach.,E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","pipe section removed and repaired in E/R workshop","2020-03-03","","Completed","2020-03-03","No","No","No","Internal"]
[null,null,null,null,12361,"38_05-May-20 4:35:09 PM","2020-03-07","Critical Equipment","Ship Staff","Ship Staff Insp.","Fire/foam isolation valve not holding in foam room","Critical Equip.","Safety / LSA / FFA","Equipment Related","","","","","Received new valve at Singapore 14th Nov 2020, Valve renewed.","2020-05-31","","Completed","2020-11-23","No","No","No","Internal"]
[null,null,null,null,12309,"38_14-Mar-20 2:56:39 PM","2020-03-13","Defect","Ship Staff","Ship Staff Insp.","Port side provision crane guard ring found detached from access ladder at one end","Deck - Machinery","Structural Condn. / WT integrity ","Equipment Related","","","","","Detached guard ring welded to the vertical ladder by carrying out hot work after office approval.","2020-03-31","","Completed","2020-03-17","No","No","No","Internal"]
[null,null,null,null,12334,"38_03/04/2020 9:57:05 PM","2020-03-13","Breakdown","Ship Staff","Ship Staff Insp.","AIS not working","Navigation - DGPS / EPFS / AIS","Navigation","Equipment Related","","","","","trouble shooting carried out, found RF cable defective, same replaced with new spare cable","2020-03-14","","Completed","2020-03-13","No","No","No","Internal"]
[null,null,null,null,12335,"38_14-Mar-20 2:52:03 PM","2020-03-13","Defect","Ship Staff","Ship Staff Insp.","Stbd midship crane,stbd jib platform grating  found wasted due to corrosion","Deck - Machinery","Structural Condn. / WT integrity ","Equipment Related","","","","","New grating received and fitted in place","2020-04-30","","Completed","2020-04-16","No","No","No","Internal"]
[null,null,null,null,12343,"38_14-Mar-20 2:54:51 PM","2020-03-13","Defect","Ship Staff","Ship Staff Insp.","Stbd midship crane grating near slew bearing grease point and used to access operating platform found holed and wasted due to corrosion.","Deck - Machinery","Structural Condn. / WT integrity ","Equipment Related","","","","","Grating renewwed.","2020-03-31","","Completed","2020-04-15","No","No","No","Internal"]
[null,null,null,null,12326,"38_03/04/2020 9:59:06 AM","2020-03-19","Breakdown","Ship Staff","Ship Staff Insp.","FWG ejector pump outlet pipe section found leaking","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Pipe section removed and repaired in E/R workshop","2020-03-20","","Completed","2020-03-20","No","No","No","Internal"]
[null,null,null,null,12332,"38_03/04/2020 9:48:06 PM","2020-03-20","Breakdown","Ship Staff","Ship Staff Insp.","Fore peak store fire alarm bell found broke","Miscellaneous","Emgcy. Systems","Equipment Related","","","","","Fire alarm bell replaced with new spare. tested found working satisfactory","2020-03-20","","Completed","2020-03-20","No","No","No","Internal"]
[null,null,null,null,12295,"38_05-May-20 4:32:30 PM","2020-03-22","Defect","Ship Staff","Ship Staff Insp.","AC room door packing and AC room door found deformed and not closing properly","Accommodation ","Safety / LSA / FFA","Equipment Related","","","","","AC room door hinges bracket were repaired by hotwork after office concurrence. Now door is closing properly.","2020-12-30","","Completed","2020-10-30","No","No","No","Internal","rectified by ship staff"]
[null,null,null,null,12327,"38_03/04/2020 10:01:56 AM","2020-03-22","Breakdown","Ship Staff","Ship Staff Insp.","EGB circulating pump coupling found broken","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","coupling replaced with new spare","2020-03-22","","Completed","2020-03-22","No","No","No","Internal"]
[null,null,null,null,12333,"38_03/04/2020 9:52:50 PM","2020-03-25","Observation","Ship Staff","Ship Staff Insp.","Emergency generator starting batteries not holding charge","LSA / FFA","Emgcy. Systems","Equipment Related","","","","","Batteries replaced with new spare batteries","2020-03-25","","Completed","2020-03-25","No","No","No","Internal"]
[null,null,null,null,12358,"38_05-May-20 4:39:31 PM","2020-03-26","Critical Equipment","Ship Staff","Ship Staff Insp.","One of the Foam hydrant adjacent to Foam monitor bound broken","Critical Equip.","Safety / LSA / FFA","Equipment Related","","","","","New hydrant put in place.","2020-05-31","","Completed","2020-04-06","No","No","No","Internal"]
[null,null,null,null,12329,"38_03/04/2020 10:05:14 AM","2020-03-27","Critical Equipment","Ship Staff","Ship Staff Insp.","Flame detector above boiler found giving false alarm","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","Flame detector replaced with new spare","2020-03-27","","Completed","2020-03-27","No","No","No","Internal"]
[null,null,null,null,12294,"38_05/05/2020 11:42:04 AM","2020-04-01","Breakdown","Ship Staff","Ship Staff Insp.","Accommodation AC no 2 , tubes  entering evaporator section have multiple leaks","Accommodation ","MLC Related","Equipment Related","","","","","Fixed new Evaporator by Shore techanician and tested. Working satisfactory","2020-06-01","","Completed","2020-06-26","No","No","No","Internal","new evaporator cole ready will be installed by technician this call fujairah"]
[null,null,null,null,null,"38_18/05/2020 17:02:32","2020-04-01","Defect","Ship Staff","Ship Staff Insp.","Oil observed leaking from valve box no.3A. The valve block for No.2 drop valve is leaking","Cargo Mach.","Cargo / Ballast Systems","Equipment Related",null,null,"Not Applicable","Not Applicable","The vlave block has to be taken out & the leak rectified. Presently, No Leak observed","2020-07-01",null,"Completed","2020-11-15","No",null,null,"Internal"]
[null,null,null,null,12331,"38_03/04/2020 9:44:31 PM","2020-04-03","Breakdown","Ship Staff","Ship Staff Insp.","S/T lub oil storage tank high level alarm found not working","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","Float inspected, found testing mechanism stuck, same eased up . alarm tried out found working satisfactory","2020-04-04","","Completed","2020-04-03","No","No","No","Internal"]
[null,null,null,null,12337,"38_16-Apr-20 1:48:23 PM","2020-04-07","Defect","Ship Staff","Ship Staff Insp.","One wire strand of port provision crane hoisting wire found broken.","Miscellaneous","General Appearance","Equipment Related","","","","","New wire received while passing galle. Same is renewed and load tested to 10T. No damage noted after testing.","2020-04-30","","Completed","2020-04-16","No","No","No","Internal"]
[null,null,null,null,12338,"38_08/04/2020 4:40:58 PM","2020-04-08","Defect","Ship Staff","Ship Staff Insp.","Emergency fire pump mechanical seal found leaking","LSA / FFA","Emgcy. Systems","Equipment Related","","","","","mechanical seal renewed","2020-04-09","","Completed","2020-04-09","No","No","No","Internal"]
[null,null,null,null,12351,"38_05-May-20 4:45:35 PM","2020-04-10","Breakdown","Ship Staff","Ship Staff Insp.","One of the window wiper on the port side found inoperational","Navigation - Others","Navigation","Equipment Related","","","","","Window wiper operating motor found kaput. same renewed. window wiper working satisfactory","2020-06-30","","Completed","2020-05-09","No","No","No","Internal"]
[null,null,null,null,12359,"38_05-May-20 4:37:44 PM","2020-04-14","Critical Equipment","Ship Staff","Ship Staff Insp.","No.2 & No.3 foam isolation valves on deck are leaking.","Critical Equip.","Safety / LSA / FFA","Equipment Related","","","","","Both valaves replaced with new valves received in fujairah","2020-06-30","","Completed","2020-05-12","No","No","No","Internal"]
[null,null,null,null,12347,"38_05-May-20 4:42:52 PM","2020-04-30","Critical Equipment","Ship Staff","Ship Staff Insp.","BNWAS inoperational","Navigation - VDR / BNWAS","Navigation","Equipment Related","","","","","Required spares or new equipment. PO rasied EAGL200190. Complete new system installed on 11 may 2020 at Fujairah by shore technician","2020-06-30","","Completed","2020-05-11","No","No","No","Internal"]
[null,null,null,null,12342,"38_05/05/2020 11:37:38 AM","2020-05-01","Breakdown","Ship Staff","Ship Staff Insp.","IG Scrubber tower metal plate wasted","Inert Gas","Eng. / Strg. Comp.","Equipment Related","","","","","New plate welded after officer approval for hot work and proper isolation","2020-05-05","","Completed","2020-05-05","No","No","No","Internal"]
[null,null,null,null,12348,"38_05/05/2020 11:33:52 AM","2020-05-05","Breakdown","Ship Staff","Ship Staff Insp.","STBD Life boat sprinkler pump casing found crack","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","Sprinkler pump replaced with complete new pump","2020-05-07","","Completed","2020-05-09","No","No","No","Internal"]
[null,null,null,null,12354,"38_05/05/2020 11:48:55 AM","2020-05-05","Breakdown,Defect","Ship Staff","Ship Staff Insp.","Sewage plant air blower outlet air flow not sufficient, fouling smell emanating from the sewage plant","Critical Equip.","MARPOL Related","Equipment Related","","","","","To inspect air blower air pipe sections for any leaks. To check vent pipe for any chocking/ Air blower inspected, all parts cleaned, sewage plant vent line checked and cleaned, now blower air pressure is sufficient.","2020-05-10","","Completed","2020-08-31","No","No","No","Internal"]
[null,null,null,null,12296,"38_06/05/2020 5:42:41 PM","2020-05-06","Breakdown","Ship Staff","Ship Staff Insp.","economizer feed water pump no 1 drawing high current","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","Economizer feed water pump no.1 dismantled, all parts inspected, all found in order, ball bearings renewed, motor overhauled. Now pump is drawing 32 amps.","2020-11-30","","Completed","2020-11-10","No","No","No","Internal","let us know once the job is completed"]
[null,null,null,null,12298,"38_18/05/2020 04:01:35","2020-05-15","Breakdown","Ship Staff","Ship Staff Insp.","In Juaymah Pilot has put the vessel on notice that vessel's air conditioning is not effective. One AC unit is out of order awaiting new evaporatore. It is all opened up","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","New Evaporator Fixed, fan impeller replaced. Gas charged. AC performing very well. outside temp above 44 deg C and accommodation 22 deg C with two AC plants running. Plant automation not working, controlled manually.","2020-06-26","","Completed","2020-06-26","No","No","No","Internal","New Evaporator is ready will be installed at Fujairah during bunkering"]
[null,null,null,null,12299,"38_18/05/2020 16:50:32","2020-05-15","Breakdown","Ship Staff","Ship Staff Insp.","On 15th May elevator stopped working whilst vessel was loading at Juaymah. It was attended by technicians in Fujairah & made operational on the 11th of May. But is not working since the 15th of May. ","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","Technician attended job at Fujairah on 26th June 2020. Cards replaced brought by techancian. Elevator made operational.","2020-07-15","","Completed","2020-06-26","No","No","No","Internal","new encoder procured by technician, will be attended next call Fujairah ."]
[null,null,null,null,12357,"38_18/05/2020 16:56:22","2020-05-15","Defect","Ship Staff","Ship Staff Insp.","During loading at Juaymah port slop tank valve opened on its own as per the CCR indicator when the switch was on neutral & loss of about 60 litres of hydraulic oil was reported.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","To check the solenoid coil for the valve, identify which valve is leaking & fix the leak. - SAME DEFECT HAS BEEN RECORDED AS DUPLICATE, ALREADY EXSITING IN THE DEFECT LIST.","2020-07-04","","Completed","2020-11-15","No","No","No","Internal"]
[null,null,null,null,15353,"38_14-Jun-20 11:49:54 PM","2020-05-16","Defect","Ship Staff","Ship Staff Insp.","NAVTEX AND X-BAND RADAR INPUTS ARE NOT BEING RECEIVED IN ECDIS","Navigation - ECDIS","Navigation","Equipment Related","4.13","Very High","","","PROBLEM DISCUSSED WITH OFFICE. ONBOARD INVESTIGATION FOUND CABLE DEFECTIVE NEW CABLE LAID DOWN AND DEFECT RECTIFIED","2020-06-30","","Completed","2020-06-30","No","No","No","Internal"]
[null,null,null,null,12353,"38_18/05/2020 11:18:31 PM","2020-05-18","Breakdown","Ship Staff","Ship Staff Insp.","Steering gear room exhaust fan motor found showing low insulation","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Inspected all in details on 30th June 2020. Found Cable damaged on Deck. Received cable on 26th June 2020. Job will be undertaken after office approval at sea and in calm weather. Requires staging in steering room. Office approval taken. Staging errected and replaced thje damaged section of wirings. Now all satisfactory.","2020-05-22","","Completed","2020-07-28","No","No","No","Internal"]
[null,null,null,null,12352,"38_22/5/2020 7:38:33 PM","2020-05-21","Defect","Ship Staff","Ship Staff Insp.","Gray water overboard pipe section just before overboard valve found leaking","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Tried to remove the pipe section but found overboard valve is not holding. Temporary repair carried out on the leaking section, permanent job to be carried out at anchorage in ballast condition","2020-06-10","","Completed","2020-06-09","No","No","No","Internal"]
[null,null,null,null,15344,"38_09-Jun-20 10:14:03 AM","2020-06-04","Defect,Observation","Ship Staff","Ship Staff Insp.","no.4 & 5 mooring winch found to be leaking from distribution valve block.","Deck - Mooring Machinery","Mooring","Equipment Related","","","","","New seal put in place and Cap nut braized to arrest  leaks. Winched tried out and found operational without any leaks. However for permanant repairs vessel has requested spares under EAGL200134, EAGL200241.","2020-09-04","","Completed","2020-06-18","No","No","No","Internal"]
[null,null,null,null,15360,"38_17/06/2020 10:38:17 AM","2020-06-05","Defect","Ship Staff","Ship Staff Insp.","Atm condenser sea water inlet end cover has water seepage marks, suspecting thinning of the material","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","At fujairah anchorage, to remove and repair Atmosferic condenser cover was open for inspection.Found all in order.Zink anodes renew and condeser chemically cleaning done.Put back for service.No leakages observe.","2020-07-07","","Completed","2020-08-12","No","No","No","Internal"]
[null,null,null,null,15389,"38_11-Jun-20 4:44:21 AM","2020-06-05","Defect","Ship Staff","Ship Staff Insp.","Bonding wires of found broken on various pipelines and fittings on deck","Miscellaneous","General Appearance","Equipment Related","","","","","Broken bonding wire are replaced with new bonding wires.","2020-06-05","","Completed","2020-10-04","No","No","No","Internal"]
[null,null,null,null,15370,"38_09-Jun-20 10:07:44 AM","2020-06-06","Observation","Ship Staff","Ship Staff Insp.","No.1 COP upper bearing temperature found to be on higher side (70 deg C). Pump wah being used for COW & pump rpm was 1050.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","Greasing of the pump bearing to be carried out and teperature to be observed again during next cargo discharging. For last 1 yr data shows bearing temp on higher side/ last discharging temperature of bearing was monitiored, temp was showing almost same as other COP bearing temperature.","2020-09-06","","Completed","2020-09-19","No","No","No","Internal"]
[null,null,null,null,15342,"38_09-Jun-20 10:11:22 AM","2020-06-06","Observation","Ship Staff","Ship Staff Insp.","No.2, 3, 6 mooring winch break found to be erratic in operation, causing lot of noise during winch operation.","Deck - Mooring Machinery","Mooring","Equipment Related","","","","","Temporary repairs carried out brake screw end grinded and threads fabricated using dies, check nut put in place. Winches tried out. For permanant repairs PO for 2 spare Brake screw for use in emergency. EAGL200241 pending.","2020-09-06","","Completed","2020-06-14","No","No","No","Internal"]
[null,null,null,null,15390,"38_11-Jun-20 4:40:57 AM","2020-06-08","Observation","Ship Staff","Ship Staff Insp.","Many safety chain hooks along the catwalk on main deck area found broken.","Deck - Pipe / Fittings","General Appearance","Equipment Related","","","","","New chain received and replaced.","2020-09-08","","Completed","2020-08-30","No","No","No","Internal"]
[null,null,null,null,null,"38_13-Jun-20 10:48:43 AM","2020-06-12","Defect","Ship Staff","Ship Staff Insp.","SART LOCKING PIN BROKEN AND MISSING","LSA / FFA","Safety / LSA / FFA","Equipment Related",null,null,"Not Applicable","Not Applicable","Locking pin fitted with temporary repairs . NEW SART RFQ RAISED","2020-09-12","EAGL200010","Completed","2020-12-10","No",null,null,"Internal"]
[null,null,null,null,15341,"38_13/06/2020 8:17:01 AM","2020-06-16","Breakdown","Ship Staff","Ship Staff Insp.","EGB circulating pump mechanical seal found leaking","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","mech seal replaced with new seal, pump tried out found working satisfactory","2020-06-17","","Completed","2020-06-16","No","No","No","Internal"]
[null,null,null,null,15345,"38_04/07/2020 11:43:40 AM","2020-06-21","Breakdown","Ship Staff","Ship Staff Insp.","DAMAGED AHU #2 BLOWER IMPELLER. REQUIRE REPLACEMENT","Accommodation ","Eng. / Strg. Comp.","Equipment Related","","","","","NEW RECEIVED AT FUJAIRAH. REPLACED BEARINGS, SHAFT AND IMELLER. TRIED OUT. ALL SATISFACTORY","2020-06-30","","Completed","2020-06-26","No","No","No","Internal"]
[null,null,null,null,15346,"38_04/07/2020 11:49:56 AM","2020-06-21","Breakdown","Ship Staff","Ship Staff Insp.","LEAK FROM SUMP SIGHT GLASS. TO REPLACE","E/R - Purifier","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","REPLACED SIGHT GLASS WITH NEW GASKETS. LEAK RECTIFIED","2020-06-22","","Completed","2020-06-22","No","No","No","Internal"]
[null,null,null,null,15348,"38_08/07/2020 10:03:11 AM","2020-06-21","Breakdown","Ship Staff","Ship Staff Insp.","MECHANICAL SEAL LEAKING OF REF #1 COMP. COMP STOPPED, ISOLATED. SEAL TO REPLACE","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","REPLACED SEAL AND SYSTEM CHECKED. LEAKAGE RECTIFIED","2020-07-08","","Completed","2020-07-08","No","No","No","Internal"]
[null,null,null,null,15350,"38_11/07/2020 8:04:23 PM","2020-06-21","Breakdown","Ship Staff","Ship Staff Insp.","Oil Leak from #1 Boiler FO Supply Pump, Excessive vibration and abnormal sound. Pump not in standby mode","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","DISMANTLED PUMP AND FOUND PUMP COUPLING FREE ON PUMP SHAFT. KEY WAY OF PUMP SHAFT DAMAGED. OVERHAULED PUMP, REPLACED SEAL, BEARINGS, COUPLINGSS. DRESS SHAFT GROOVE AND FABRICATED KEY ONBOARD. AFTER ASSEMBLING PUMP TRIED OUT, PERFORMANCE SATISFACTORY.","2020-07-10","","Completed","2020-07-11","No","No","No","Internal"]
[null,null,null,null,15343,"38_24/6/2020 9:29:48 PM","2020-06-23","Breakdown","Ship Staff","Ship Staff Insp.","Ballast Pump #2 upper Bearing temp. Sensor faulty","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.8","Medium","","","Replaced with spare sensor unit","2020-06-24","","Completed","2020-06-23","No","No","No","Internal"]
[null,null,null,null,15347,"38_08/07/2020 10:00:31 AM","2020-06-25","Breakdown","Ship Staff","Ship Staff Insp.","MAIN ENGINE FO CIR PUMP #1 ABNORMAL NOISE FROM PUMP AND SEAL LEAKING","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","PUMP DISMANTLED, FOUND DAMAGED BEARINGS, SPIDER DAMAGED. REPLACED BEARINGS, MECH SEAL AND SPIDER. PUMP TRIED OUT PERFORMANCE SATISFACTORY.","2020-07-09","","Completed","2020-07-07","No","No","No","Internal"]
[null,null,null,null,15369,"38_10-Jul-20 3:23:20 PM","2020-07-04","Defect","Ship Staff","Ship Staff Insp.","During loading/deballasting at rastanura observed pin hole at No.2 Ballast pump discharge valve BA542F. ","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","Ballast discharge valve replaced with new valve received on board and checked for operation on 30 -Aug-2020, and now opeartional and satisfactory","2020-10-30","EAGL200273","Completed","2020-08-30","No","No","No","Internal"]
[null,null,null,null,15359,"38_09-Jul-20 2:12:53 PM","2020-07-04","Defect","Ship Staff","Ship Staff Insp.","S-VDR onboard having issue with port bridge wing microphone. \n\nAlarm is active stating ‘AUDIO ERROR microphone test failed’\n\nAlarm 2(2) ERROR CODE 4632\n\n","Navigation - VDR / BNWAS","Navigation","Equipment Related","","","","","Upon investigating vessel found VDR MIC (port wing) was Faulty. Same were received and replaced. alarm reseted. VDR backup taken and all individual mic recording verified. system working satisfactory.","2020-08-04","EAGL205050","Completed","2020-07-31","No","No","No","Internal"]
[null,null,null,null,15349,"38_8/7/2020 7:51:21 PM","2020-07-05","Breakdown,Critical Equipment","Ship Staff","Ship Staff Insp.","SLUGGISH OPERATION OF PRIMING UNIT OF EMERGENCY FIRE PUMP, ALSO LEAKING WHEN PUMP STARTING","Critical Equip.","Eng. / Strg. Comp.","Equipment Related","5.41","Very High","","","during loaded passage Pump unit Overhauled after office approval. Pump can take suction without priming unit during loaded passage. Seals/ Bearings replaced. System operational without any leak","2020-07-08","","Completed","2020-07-08","No","No","No","Internal"]
[null,null,null,null,15371,"38_22/09/2020 17:15:18","2020-07-12","Critical Equipment","Ship Staff","Ship Staff Insp.","DAMAGED AIR SHUT OFF VALVE FOR ENGINE ROOM FAN AND FUNNEL DAMPERS","Critical Equip.","Emgcy. Systems","Equipment Related","5.35","Medium","","","REQUISTION NO. EAGL200243 WAS RAISED EARLIER. AFTER RECEIVING THE NEW AIR SHUT OFF VALVE, VALVE WAS REPLACED WITH NEW VALVE.","2020-10-20","","Completed","2020-09-22","No","No","No","Internal"]
[null,null,null,null,15358,"38_13/07/2020 4:23:44 PM","2020-07-13","Breakdown","Ship Staff","Suptd. Insp.","FLAME SENSOR ON TOP OF MAIN ENGINE AFT SIDE FOUND NOT WORKING","Critical Equip.","Safety / LSA / FFA","Equipment Related","5.39","Very High","","","FIRE SENSOR REPLACED WITH ONBOARD SPARE AFTER TAKING APPROVAL FOR WORKING ALOFT AND PERMIT TO WORK ON CRITICAL EQUIPMENT. SYSTEM TRIED OUT, ALL SATISFACTORY.","2020-07-13","","Completed","2020-07-13","No","No","No","Internal"]
[null,null,null,null,15366,"38_15/07/2020 5:32:34 PM","2020-07-14","Breakdown","Ship Staff","Ship Staff Insp.","Ballast Pump #2 Mechanical Seal Leaking","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.15","High","",""," Received new spare mechanical seal, old mechanical seal was replaced with new one, now no leak.","2020-08-15","EAGL200280","Completed","2020-08-03","No","No","No","Internal"]
[null,null,null,null,15351,"38_15/07/2020 5:23:53 PM","2020-07-14","Breakdown","Ship Staff","Ship Staff Insp.","PRESSURE READING ERRATIC IN CCR AND ALL REMOTE STATIONS","Critical Equip.","Cargo / Ballast Systems","Equipment Related","8.25","Very High","","","INVESTIGATED IN DETAILS  AND FOUND PRESSURE TRANSMITTER IN PUMP ROOM 6.32 DEFECTIVE. SAME REPLACED WITH ONBOARD SPARE. CHECKED PERFORMANCE, ALL SATISFACTORY.","2020-07-15","","Completed","2020-07-15","No","No","No","Internal"]
[null,null,null,null,15355,"38_18/07/2020 5:15:53 PM","2020-07-14","Breakdown","Ship Staff","Ship Staff Insp.","Drain Pipe of Emgcy gen. natural vent chocked. water can overflow and fall on Alternator","Miscellaneous","Structural Condn. / WT integrity ","Equipment Related","10.23","Medium","","","Pipe Sections removed. Pipe holed / damaged. Chocked sections cleared. salt deposits in tray cleared. In place pipe repaired by cold means. System restored vback to normal","2020-07-20","","Completed","2020-07-18","No","No","No","Internal"]
[null,null,null,null,15354,"38_19/07/2020 9:22:04 PM","2020-07-17","Breakdown","Ship Staff","Ship Staff Insp.","ONE OF WINDOW WIPER NON OPERATIONAL","Navigation - Others","Navigation","Equipment Related","12.1","High","","","REMOVED COMLETE FITTING, REPLACED WIPER CAM, GUIDES, BELTS. SYSTEM MADE OPERATIONAL","2020-07-19","","Completed","2020-07-19","No","No","No","Internal"]
[null,null,null,null,15352,"38_18/07/2020 5:21:09 PM","2020-07-18","Breakdown","Ship Staff","Ship Staff Insp.","IG SAMPLING LINE DAMAGED GOING TO OXYGEN ANALYZER IN ENGINE ROOM","Inert Gas","Cargo / Ballast Systems","Equipment Related","8.25","Very High","","","SAMPLING LINE RENEWED, ALSO NOTICED PICK UP HOLE FOR IG SAMPLE CHOCKED. SAME CLEARED AND SYSTEM MADE OPERATIONAL","2020-07-18","","Completed","2020-07-18","No","No","No","Internal"]
[null,null,null,null,15356,"38_23/7/2020 4:41:46 PM","2020-07-19","Breakdown","Ship Staff","Ship Staff Insp.","Found spark arrestor of Emergency Generator exhaust manifold errroded and damaged. Required tro replace","Critical Equip.","Safety / LSA / FFA","Equipment Related","10.32","Very High","","","Removed front silencer and fabricated new onboard and fixed back.","2020-07-24","","Completed","2020-07-23","No","No","No","Internal"]
[null,null,null,null,15357,"38_29/07/2020 10:34:22 AM","2020-07-27","Breakdown","Ship Staff","Ship Staff Insp.","440 VOLTS LOW INSULATION FROM EMERGENCY FIRE PUMP ROOM EXHAUST FAN. ","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.38","Medium","","","INTIALLY SYSTEM ISOLATED. FOUND WIRINGS ON WEATHER DECK DAMAGED. OFFICE APPROVAL TAKEN TO WORK ALOFT AND REPLACED THE DAMAGED SECTION OF WIRING AFTER OPENING PENTRATION OF WIRE. SYSTEM CHECKED. ALL SATISFACTORY. OFFICE UPDATED","2020-07-29","","Completed","2020-07-28","No","No","No","Internal"]
[null,null,null,null,15361,"38_29/08/2020 14:17:40","2020-08-04","Defect","Ship Staff","Ship Staff Insp.","STEAM LEAK FROM EGB STEAM SOOT BLOW INLET VALVE GASKET","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.19","Very High","","","STEAM ISOLATED, STEAM VALVE INLET FLANGE AND VALVE BONNET GASKET RENEWED.","2020-08-15","","Completed","2020-08-10","No","No","No","Internal"]
[null,null,null,null,15363,"38_29/08/2020 14:29:25","2020-08-12","Defect","Ship Staff","Ship Staff Insp.","LUB OIL LEAK FROM ME LUB OIL AUTO BACKWASH FILTER OUTLET VALVE FLANGE GASKET","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.19","Very High","","","AUTO BACKWASH FILTER OUTLET VALVE FLANGE GASKET WAS RENEWED, NOW NO LEAK. ","2020-08-31","","Completed","2020-08-19","No","No","No","Internal"]
[null,null,null,null,15362,"38_29/08/2020 14:24:42","2020-08-17","Defect","Ship Staff","Ship Staff Insp.","WATER LEAK FROM IG SCRUBBER SIGHT GLASS TUBE","Inert Gas","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","SCRUBBER SIGHT GLASS TUBE WAS REPLACED WITH NEW ONE, NOW NO LEAK.","2020-08-31","","Completed","2020-08-18","No","No","No","Internal"]
[null,null,null,null,15364,"38_30/08/2020 8:01:16","2020-08-27","Defect","Ship Staff","Ship Staff Insp.","NO.2 AE OIL MAX PUMP OIL SEAL LEAK","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","NO.2 AE OIL MAX PUMP OIL SEALS RENEWED. NOW NO LEAK OBSERVED.","2020-08-31","","Completed","2020-08-28","No","No","No","Internal"]
[null,null,null,null,15365,"38_31-Aug-20 12:18:21 PM","2020-08-29","Defect","Ship Staff","Ship Staff Insp.","During bridge watch duty officer observed AIS Showing below alertS:- 1. AIS TX POWER TOO LOW , 2. AIS ANTENNA VSWR EXCEEDS LIMIT,  3. AIS TX MALFUNCTION.  and noticed other vessels in vicinity is unable to see own vessel on AIS.","Navigation - DGPS / EPFS / AIS","Navigation","Equipment Related","","","","","Vessel checked the AIS antenna, connector and cable. connector removed, cleaned with contact cleaner and reconnected and AIS Restarted. currently ais working fine with NO errors.","2020-09-14","","Completed","2020-08-31","No","No","No","Internal"]
[null,null,null,null,15367,"38_10/09/2020 2:33:58 PM","2020-09-03","Critical Equipment,Non Conformity","Ship Staff","Ship Staff Insp.","PURIFIER ROOM HIGH EXPANSION PIPES FOUND WASTED.","Critical Equip.,LSA / FFA","Safety / LSA / FFA","Equipment Related","5.35","Medium","","","WASTED FOAM PIPES REMOVED FROM PLACE AND NEW PIPES WERE FABRICATED AND FITTED BACK. OFFICE CONCURRENCE WAS TAKEN.","2020-09-10","","Completed","2020-09-06","No","No","No","Internal"]
[null,null,null,null,15368,"38_10/09/2020 2:47:51 PM","2020-09-08","Defect","Ship Staff","Ship Staff Insp.","NO.2 AUX BOILER STEAM ATOMISING VALVE WAS LEAKING FROM GLAND PACKING","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.19","Very High","","","ATOMISING VALVE OVERHAULED, GLAND PACKING RENEWED AND FITTED BACK, NOW NO LEAK DETECTED.","2020-09-15","","Completed","2020-09-09","No","No","No","Internal"]
[null,null,null,null,15376,"38_22/09/2020 12:35:49","2020-09-16","Breakdown","Ship Staff","Ship Staff Insp.","ME JACKET FW PUMP MOTOR NO.2 BURNT OUT.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","NEW ELECTRICAL MOTOR RECEIVED AND SAME WAS REPLACED WITH OLD MOTOR.","2020-11-15","REQU. NO.- EAGL200310","Completed","2020-10-09","No","No","No","Internal"]
[null,null,null,null,15372,"38_05-Oct-20 10:02:47 AM","2020-09-17","Observation","FSC Inspector","OM Insp. (Eg. SIRE / CDI etc.)","LIFE BOAT MARKING FOUND FOULED ON TOP SIDE OF THE BOAT AND NO OF THE LIFEBOAT THEY SERVE NOT MARKED","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.31","High","","","LIFE  BOAT MARKING  IN SEQUENCE THEY REPRESENT ONBOARD IN NUMERICAL ORDER REQUIRED TO BE MARKED.LIFE BOAT MARKED ARE COMPLETED AS PER REQUIRMENTS.","2020-09-28","","Completed","2020-09-27","No","No","No","External"]
[null,null,null,null,15373,"38_05-Oct-20 10:09:50 AM","2020-09-17","Observation","FSC Inspector","OM Insp. (Eg. SIRE / CDI etc.)","BALLAST TANK VENT HEADS COVER FOUND CORRODED OF 3P WBT &  4S WBT","Deck - Pipe / Fittings","Cargo / Ballast Systems","External Factors","11.7","High","","","NEW COVER REQUIRED TO FABRICATE ON VENT HEAD OF 3P & 4S WBT . NOTE: NEW FARRICATED COVER OF TANK VENT HEAD FITTED ON BALLAST TANK VENT HEAD OF 3P WBT & 4S WBT, BOTH VENTS NOW SATISFACTORY.","2020-09-28","","Completed","2020-09-27","No","No","No","External"]
[null,null,null,null,15377,"38_22/09/2020 12:44:03","2020-09-18","Defect","Ship Staff","Ship Staff Insp.","DURING CARGO DISCHARGING OPERATION, FOUND WATER LEAK FROM IG SCRUBBER FLUE GAS INLET PIPE, JUST BELOW THE EXPANSION BELLOW.","Inert Gas","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","",""," NEW EXPANSION BELLOW WAS RECEIVED AND REPLACED WITH OLD DAMAGED BELLOW AND DAMAGED PIPE WAS REPAIRED BY INPLACE WELDING.","2020-10-31","","Completed","2020-10-07","No","No","No","Internal"]
[null,null,null,null,15374,"38_21-Sep-20 11:28:52 PM","2020-09-20","Breakdown","Ship Staff","Ship Staff Insp.","STBD BRIDGE WING GYRO REPEATER IS SHOWING WRONG HEADING. SYNCHRONIZATION BUTTON NOT WORKING AND IN BAD CONDITION.","Navigation - Others","Navigation","Equipment Related","","","","","VESSEL HAS SPARE GYRO REPEATER, SAME WILL PE REPLACE IN LIEU OF FAULTY ONE. NOTE: FAULTY GYRO REPEATER HAS BEEN REPLACED WITH NEW ONE ON 30-SEPT-2020 DURING ANNUAL SERVICE AT SINGAPORE .","2020-12-20","","Completed","2020-09-30","No","No","No","Internal"]
[null,null,null,null,15375,"38_22/09/2020 12:24:42","2020-09-21","Critical Equipment","Ship Staff","Ship Staff Insp.","ENGINE ROOM PORT SIDE HIGH EXPANSION FOAM LINE DAMAGED , LOCATION UNDER THE TOP OF ER CEILING, PIPE SIZE 125A.","Critical Equip.","Safety / LSA / FFA","Equipment Related","5.35","Medium","","","WASTED FOAM PIPES WERE REMOVED AND NEW PIPES WERE FABRICATED AND FITTED BACK.","2020-10-31","REQU. NO.- EAGL200322","Completed","2020-10-28","No","No","No","Internal"]
[null,null,null,null,null,"38_22/09/2020 15:57:52","2020-09-21","Defect","Ship Staff","Ship Staff Insp.","OIL LEAK FROM NO.2 COP MAIN L.O.PUMP OIL SEAL ","Cargo Mach.","Cargo / Ballast Systems","Equipment Related",8.8000000000000007,"Medium","Not Applicable","Not Applicable","OIL SEAL HAS BEEN RENEWED AND NO OIL LEAK WAS OBSERVED.","2020-12-20","Requisition no. EAGL200321 RCVD ON BOARD AT FUJAIRAH 06 December 2020.","Completed","2020-12-10","No",null,null,"Internal"]
[null,null,null,null,15378,"38_30-Oct-20 11:04:36 AM","2020-09-30","Non Conformity","Owner / Marine / Tech. Suptd.","ISPS Audit","Stbd anchor was in use however the hawse pipe cover was not secured. This is in violation of Safety Flash #102.","Deck - Machinery","ISPS Related","Human Error","","","","","Hawse pipe was secured immediately , and crew member was called and briefed about this non compliance. Proper training to crew as per vessel standard operating procedure.\n\nSenior officer shall delegate task to junior officers and crew members in such manner as to reduce workload and fatigue.","2020-12-28","","Completed","2020-10-02","No","No","No","Internal"]
[null,null,null,null,15379,"38_30/10/2020 16:06:53","2020-09-30","Non Conformity","FSC Inspector","Flag State Insp.","The funnel fire flaps failed to close fully when activated by ship staff. considerable amount of gap were noticed within the louvers.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.18","High","","","The funnel flaps free movements was check,old grease was removed,funnel links were lubricated and air cylinder stroke was adjusted. Now funnel flaps are closing properly.","2020-10-29","","Completed","2020-10-01","No","No","No","External"]
[null,null,null,null,15380,"38_30/10/2020 16:14:47","2020-09-30","Non Conformity","Owner / Marine / Tech. Suptd.","ISM Audit","One webbing slings and one wire sling found damaged in E/R.","Miscellaneous","ISM Related","Equipment Related","10.28","Low","","","All the loose gears and equipment were checked and inspected as per company procedures and damaged loose gears were discarded and removed from the inventory.","2020-12-28","","Completed","2020-10-06","No","No","No","Internal"]
[null,null,null,null,15383,"38_31-Oct-20 3:01:40 AM","2020-09-30","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","The face mask of the fireman suits does not cover all skin areas like the person’s ears area.","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.43","High","","","All fireman's outfit onboard checked for the shortcomings identified and required requisition has been raised for replacement of same. REQUISITION HAS BEEN RECEIVED AND SAME NOW IN USE FIREMANS SUIT ARE IN PROPER ORDER NOW","2020-12-28","","Completed","2020-10-21","No","No","No","Internal"]
[null,null,null,null,15388,"38_31-Oct-20 2:59:32 AM","2020-09-30","Non Conformity","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Air leak was noted at the following locations:\n\n- Port side gangway\n\n- Main deck @ 5C COT\n\n- Aft of accommodation block b-deck.","Miscellaneous","Structural Condn. / WT integrity ","Equipment Related","","","","","Requisition for air valve for replacement onboard will be raised and shall be renewed as received onboard. OLD VALVES HAS BEEN REPLACED WITH NEW ONE ONBOARD AND NOW NO LEAK OBSERVED .","2020-12-28","","Completed","2020-10-28","No","No","No","Internal"]
[null,null,null,null,null,"38_30/10/2020 16:18:46","2020-09-30","Observation","Owner / Marine / Tech. Suptd.","ISM Audit","Gas welding hose is secured to the torch using two jubilee clips. The securing to be carried out by crimping.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related",5.26,"Medium","Not Applicable","Not Applicable","Crimping connection and tools from Unitor supplie was RCVD on board at Fujairah 06 December 2020. The Oxygen & Acetylene hose has been connecting by crimping tools.","2020-12-28","EAGL 200342 RCVD on board at 06 December 2020 at Fujairah.","Completed","2020-12-08","No",null,null,"Internal"]
[null,null,null,null,null,"38_31-Oct-20 2:38:54 AM","2020-09-30","Non Conformity","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Walkie talkies were not carried in accordance with Safety Flash 85 of 2018 “Use and abuse of walkie-talkies on ships”.","Miscellaneous","Communication","Human Error",null,null,"Not Applicable","Not Applicable","All ship staff immediately briefed about such violation and made them aware about use of walkie talkie and handling them safely, also safety flash discussed 85 of 2018,and associated guidelines provided there in. Required holsters received.","2020-12-30","EAGL 200347","Completed","2020-12-06","No",null,null,"Internal"]
[null,null,null,null,null,"38_31-Oct-20 2:40:57 AM","2020-09-30","Non Conformity","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Fireman’s outfit flash lights are not explosion proof.","LSA / FFA","Safety / LSA / FFA","Equipment Related,Human Error",5.43,"High","Not Applicable","Not Applicable","Received explosion proof Flashlight.","2020-12-28","EAGL200364","Completed","2020-12-06","No",null,null,"Internal"]
[null,null,null,null,null,"38_31-Oct-20 2:42:51 AM","2020-09-30","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Oil level sight glass found obscure on multiple winches.","Deck - Mooring Machinery","Mooring","Equipment Related",9.14,"Medium","Not Applicable","Not Applicable"," Obscured Oil level sight glass renewed.","2020-12-28",null,"Completed","2020-11-24","No",null,null,"Internal"]
[null,null,null,null,null,"38_15/11/2020 15:02:06","2020-09-30","Defect","Owner / Marine / Tech. Suptd.","ISM Audit","Air leak was noted at the following locations:\r\n\r\n- Port side gangway\r\n\r\n- Main deck @ 5C COT\r\n\r\n- Aft of accommodation block b-deck.","Miscellaneous","Structural Condn. / WT integrity ","Equipment Related",11.4,"Very High","Not Applicable","Not Applicable","Leasks rectified, Valves repaired/ renewed. ","2020-12-30",null,"Completed","2020-10-28","No",null,null,"Internal"]
[null,null,null,null,15382,"38_31-Oct-20 3:03:26 AM","2020-10-21","Non Conformity","Ship Staff","Ship Staff Insp.","Anchor equipment found in poor condition. Insufficient lubrication on windlass. Engaging lever broke during anchoring operations due to heavy corrosion.","Deck - Mooring Machinery","Mooring","Equipment Related","9.2","Very High","","","Through greasing carried out of anchor windlass and associated fittings, break lining checked and gear lever fabricated back to windlass with new stainless steel bolts and fully operational now.","2020-11-30","","Completed","2020-10-27","No","No","No","Internal"]
[null,null,null,null,15381,"38_31-Oct-20 3:05:39 AM","2020-10-25","Non Conformity","Ship Staff","Ship Staff Insp.","Deck log book filled up by Deck Cadet.","Documentation","ISM Related","Human Error","","","","","DECK CADET HAS BEEN BRIEFED THAT HE IS NOT ALLOWED TO WRITE LOGBOOKS  , ALL OOW BY HIMSELF SHALL DO ALL RECORD KEEPING IN DECK LOG BOOK.","2020-11-25","","Completed","2020-10-28","No","No","No","Internal"]
[null,null,null,null,15397,"38_30/10/2020 9:41:01","2020-10-28","Observation","Owner / Marine / Tech. Suptd.","ISM Audit","IN FEW MOORING WINCHES OIL LEVEL IS NOT VISIBLE FROM SIGHT GLASS ","Deck - Mooring Machinery","Mooring","Equipment Related","9.14","Medium","",""," FOUR MOORING WINCHES OIL LEVEL SIGHT GLASS CHANGED. FOR REMAING THREE, REQUISITION HAS BEEN RAISED.","2020-11-28","EAGL200360","Completed","2020-11-18","No","No","No","Internal"]
[null,null,null,null,null,"38_15/11/2020 15:16:36","2020-11-01","Defect","Ship Staff","Ship Staff Insp.","Poor condition of mooring winches, lack of lubrication, Levers corroded and wasted.","Deck - Machinery","Mooring","Equipment Related",9.14,"Medium","Not Applicable","Not Applicable","Frozen arms, levers dismantled, freed-up and lubricated. New Gear Engaging levers fabricated and fitted. Thorough greasing carried out.","2021-01-01",null,"Completed","2020-12-10","No",null,null,"Internal"]
[null,null,null,null,null,"38_29-Nov-20 5:41:36 PM","2020-11-01","Non Conformity","Ship Staff","Ship Staff Insp.","Poor condition of mooring winches, lack of lubrication, Levers corroded and wasted.","Deck - Mooring Machinery","Mooring","Equipment Related",9.14,"Medium","Not Applicable","Not Applicable","Frozen arms, levers dismantled, freed-up and lubricated. New Gear Engaging levers fabricated and fitted. Thorough greasing carried out.","2021-02-01",null,"Completed","2020-12-10","No",null,null,"Internal"]
[null,null,null,null,15385,"38_12/11/2020 15:01:18","2020-11-02","Observation","Ship Staff","Ship Staff Insp.","STEAM LEAK FROM ATMOSPHERIC DUMP CONDENSER STEAM INLET VALVE BONNET ","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","ATMOSPHERIC DUMP CONDENSER STEAM INLET VALVE BONNET GASKET WAS DAMAGED, SAME WAS REPLACED, NOW NO STEAM LEAK OBSERVED.","2020-11-30","","Completed","2020-11-12","No","No","No","Internal"]
[null,null,null,null,15386,"38_15/11/2020 15:10:39","2020-11-02","Critical Equipment,Non Conformity","Ship Staff","Ship Staff Insp.","Lifeboat Food ration packets damaged - Vaccum Seal Broken","LSA / FFA","Safety / LSA / FFA","External Factors","5.28","Very High","","","Received new Food Ration Packets - Replaced with damaged ones.","2020-12-02","","Completed","2020-11-15","No","No","No","Internal"]
[null,null,null,null,15402,"38_29-Nov-20 5:47:34 PM","2020-11-02","Non Conformity","Ship Staff","Ship Staff Insp.","Lifeboat food packets damaged - Vaccum Seal broken. ","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","Urgent RO raised. Received Food Ration Packets at Singapore and Replaced","2020-12-02","EAGL200368","Completed","2020-11-15","No","No","No","Internal"]
[null,null,null,null,15403,"38_29-Nov-20 6:40:05 PM","2020-11-02","Non Conformity","Ship Staff","Ship Staff Insp.","while routine inspection of emergency escape tunnel of engine room, heaving rope found broken.","LSA / FFA,Miscellaneous","Safety / LSA / FFA","Equipment Related","","","","","Emergency escape pulley rope was replaced with spare rope.","2021-02-02","","Completed","2020-11-02","No","No","No","Internal"]
[null,null,null,null,15387,"38_16/11/2020 22:52:36","2020-11-03","Defect","Ship Staff","Ship Staff Insp.","MGPS DISPLAY ASSEMBLY IS NOT SHOWING CORRECT READING.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","NEW MGPS DISPLAY ASSEMBLY RECEIVED, SAME WAS FITTED AND NOW SHOWING CORRECT READING","2020-12-31","","Completed","2020-11-15","No","No","No","Internal"]
[null,null,null,null,15384,"38_12/11/2020 14:55:52","2020-11-07","Observation","Ship Staff","Ship Staff Insp.","STEAM LEAK FROM COP STEAM LINE BELLOW","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","BELLOW WAS REPLACED WITH SPARE BELLOW, NOW NO LEAK OBSERVED.","2020-11-30","","Completed","2020-11-12","No","No","No","Internal"]
[null,null,null,null,15391,"38_18/11/2020 3:17:48 PM","2020-11-13","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Main engine Backwash filter in operating DP mode","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Main engine lub oil backwash filters cleaned, now working satisfactory.","2020-11-18","","Completed","2020-11-16","No","No","No","Internal"]
[null,null,null,null,15392,"38_18/11/2020 3:26:47 PM","2020-11-13","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","service air compressor showing false alarm as running hours not updated   ","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Oil filter last change running hours was updated in service air comressor panel","2020-11-20","","Completed","2020-11-18","No","No","No","Internal"]
[null,null,null,null,15393,"38_18/11/2020 3:37:26 PM","2020-11-13","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ME jacket water controller is recently installed with new EPCOM unit, but found not in use & bypassed, Root cause for same to be investigated as mech part is found to be operating when moved manually","Deck - Pipe / Fittings,E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Jacket water controller to overhauled,one air pipe was leaking, now controller is working satisfactory.","2020-11-30","","Completed","2020-11-16","No","No","No","Internal"]
[null,null,null,null,15394,"38_18/11/2020 3:22:52 PM","2020-11-13","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","No.2 ME exhaust v/v cooling water o-ring leaking","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","ME Exhaust valve no.2 removed from place, valve seat o-rings replaced, exhaust valve boxed back. Now no leak observed.","2020-12-12","","Completed","2020-11-21","No","No","No","Internal"]
[null,null,null,null,15395,"38_18/11/2020 3:11:33 PM","2020-11-13","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","No.2 AHU bottom plate & insulation (portside) damaged leading to air leakage","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Same was repaired with new plate & revitting","2020-12-12","","Completed","2020-11-17","No","No","No","Internal"]
[null,null,null,null,15398,"38_18/11/2020 3:14:43 PM","2020-11-13","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","No.1 AHU water Drain Pipe is choked due to which water sipping out from AHU unit","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Drain pipe removed, pipe found choked, same cleared and fitted back.","2020-11-23","","Completed","2020-11-18","No","No","No","Internal"]
[null,null,null,null,15399,"38_18-Nov-20 6:33:12 PM","2020-11-13","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Big rust patch observed near 2S PV breaker, same to be immediately grit blast.","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.3","Medium","","","Grit blating of the rust patch carried out. other areas in progress","2020-11-18","","Completed","2020-11-25","No","No","No","Internal"]
[null,null,null,null,15400,"38_18-Nov-20 7:08:05 PM","2020-11-13","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Port side gangway top ladder Badly rusted, same to be derusted & painted.","Deck - Machinery","General Appearance","Equipment Related","5.47","Medium","","","Top ladder found corroded and wasted, same renewed and attached with nut/ bolt arrangement. Also Stbd side renewed.","2020-11-28","","Completed","2020-11-24","No","No","No","Internal"]
[null,null,null,null,15401,"38_19-Nov-20 2:12:40 AM","2020-11-13","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Suez cabin bedding left in shabby condition after last report, same to be cleaned & kept ready for usage","Accommodation ","General Appearance","Human Error","11.13","Low","","","All spare cabins including suez cabins cleaned and good housekeeping maintained after departure port. ","2020-11-14","","Completed","2020-11-15","No","No","No","Internal"]
[null,null,null,null,null,"38_18/11/2020 3:34:12 PM","2020-11-13","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","No.3 DG reported to be having high Lube oil consumption, root cause to find & rectify.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Cylinder head valve guide o-rings was renewed and breather sump tank valve was O/H.Presently everage luboil consumption for Aux.Engine No:3 about 30 ltrs per day.","2020-11-30",null,"Completed","2020-12-03","No",null,null,"Internal"]
[null,null,null,null,null,"38_18-Nov-20 6:53:56 PM","2020-11-13","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","All the defect related to Docking jobs which are updated in DDRL have to added in REFMAN,","Documentation","Cert. & Docu.","Equipment Related",null,null,"Not Applicable","Not Applicable","Vessel has been identify and move docking related jobs from DDRL to REFMAN.","2021-01-02",null,"Completed","2020-12-10","No",null,null,"Internal"]
[null,null,null,null,null,"38_18/11/2020 3:41:34 PM","2020-11-13","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","All DG camcase Inspection & tappet cover bolt tightening inspection to be carried out immediately as shown to 3rd engineer. Same to be followed every 250 hrs. All spare camcase to check & make sure one of each type is present onboard","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","All DG camcase inspections was carried out, tappet cover bolt tightening has been check.The task will be followed every 250 hrs.","2020-11-30",null,"Completed","2020-12-08","No",null,null,"Internal"]
[null,null,null,null,null,"38_18-Nov-20 6:21:56 PM","2020-11-13","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Fwd. Hydraulic priming chamber was found empty of oil which could lead to ingress of air in system, procedure to be explained to all deck personnel for filling, maintaining level at all times & starting of Hyd. System, add this level check in Pre arrival checklist as well.","Deck - Machinery","Mooring","Equipment Related",9.14,"Medium","Not Applicable","Not Applicable","Forward hydraulic machinery priming chamber to be refilled with hydraulic oil. Levels to be inspected prior every arrival so as to maintain proper oil level at all times. Deck officers has been trained for checking oil level & filling procedure of priming tanks.Importance of oil level in priming tanks to be expalined during such training.","2020-11-18",null,"Completed","2020-12-09","No",null,null,"Internal"]
[null,null,null,null,null,"38_18-Nov-20 6:27:02 PM","2020-11-13","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Order new non-return v/v from Fwd hyd. storage tank filling line to priming tank & presently put a blank in line then monitor if level in the priming tank maintains","Deck - Machinery","Mooring","Equipment Related",9.14,"Medium","Not Applicable","Not Applicable","The feelling line for  priming tank of  Fwd Hydraulic machinery equipped with stop ball valve,same to be kept in closed position to avoid oil drain back from priming tank to storage tank and to be open in case of topping oil to priming tank.","2020-12-13",null,"Completed","2020-12-09","No",null,null,"Internal"]
[null,null,null,null,null,"38_19-Nov-20 2:18:27 AM","2020-11-13","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Aft funnel has 2 big rust Rust peeling marks, same to be removed using rust stain remover after rigging staging.","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","Equipment Related",8.6300000000000008,"High","Not Applicable","Not Applicable","Deruting, painting and removal of rust stains completed. Work aloft approval obtained from office.","2020-12-13",null,"Completed","2020-12-08","No",null,null,"Internal"]
[null,null,null,null,null,"38_18-Nov-20 7:10:10 PM","2020-11-13","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Both Provision cranes have Rust peeling mark, same to be removed using rust stain remover.","Deck - Machinery","General Appearance","Equipment Related",8.6300000000000008,"High","Not Applicable","Not Applicable","Both Provision cranes Rust peeling mark removed.","2020-12-13",null,"Completed","2020-12-04","No",null,null,"Internal"]
[null,null,null,null,null,"38_18-Nov-20 7:00:32 PM","2020-11-13","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Both Midship cranes have Rust peeling mark, same to be removed using rust stain remover, spare hoses consumed to be replenished with new, order RO for hose as required","Deck - Machinery","Cargo / Ballast Systems","Equipment Related",8.6300000000000008,"High","Not Applicable","Not Applicable","Both Midship cranes have Rust peeling mark,  removed using rust stain remover, spare hoses onboard.","2020-12-13",null,"Completed","2020-12-02","No",null,null,"Internal"]
[null,null,null,null,null,"38_18-Nov-20 6:49:32 PM","2020-11-13","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Damaged Grating to change on port side manifold Between 1 & 2 Cargo line.","Deck - Pipe / Fittings","MARPOL Related","Equipment Related",6.6,"Medium","Not Applicable","Not Applicable","Gratings renewed.","2020-12-13","EAGL200388","Completed","2020-12-10","No",null,null,"Internal"]
[null,null,null,null,null,"38_19-Nov-20 2:15:29 AM","2020-11-13","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Cockroach fumigation to be carried out daily in night time in galley.","Accommodation ","General Appearance","External Factors",11.13,"Low","Not Applicable","Not Applicable","In progress - Done Daily,  number of cockroaches have reduced.","2020-11-14",null,"Completed","2020-12-10","No",null,null,"Internal"]
[null,null,null,null,15404,"38_29-Nov-20 6:45:47 PM","2020-11-15","Non Conformity","Ship Staff","Ship Staff Insp.","Mandatory placards required to display at Garbage collection stations, are missing.","Miscellaneous","MARPOL Related","External Factors","","","","","Routine inspection shall be carried out at regular basis. Required posters put on display.","2021-02-15","","Completed","2020-11-16","No","No","No","Internal"]
[null,null,null,null,15396,"38_28/11/2020 2:47:16 PM","2020-11-26","Observation","Ship Staff","Ship Staff Insp.","Fwd L.T. Cooler sea water inlet pipe leak","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Fwd L.T. Cooler was isolated and damaged sea water pipe was removed from place and brought to workshop. Pipe was repired by welding, pipe was fitted back in place and put back in service. Now no leak observed.","2020-11-30","","Completed","2020-11-27","No","No","No","Internal"]

{"sheet":"Calc","index":2,"n_rows":28,"n_cols":12,"rows_kept":28,"cut":false,"hidden":true,"merged":[]}
["Def_type","Def_cause","Equipments","VIQrefno","Observer_code"]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,"Dim itemSele As Long"]
[null,null,null,null,null,null,null,null,null,null,null,"   dim startRow as integer"]
[null,null,null,null,null,null,null,null,null,null,null,"   startRow=1"]
[null,null,null,null,null,null,null,null,null,null,null,"        For itemSele = 0 To ListBox1.ListCount - 1"]
[null,null,null,null,null,null,null,null,null,null,null,"        If ListBox1.Selected(itemSele) = True Then"]
[null,null,null,null,null,null,null,null,null,null,null,"        Worksheets(\"WorksheetName\").Range(\"A\" & startRow).Value = ListBox1.List(itemSele)"]
[null,null,null,null,null,null,null,null,null,null,null,"        startRow = startRow + 1"]
[null,null,null,null,null,null,null,null,null,null,null,"        End If"]
[null,null,null,null,null,null,null,null,null,null,null,"        Next"]
[null,null,null,null,null,null,null,null,null,null,null,"Dim LastRowA As String"]
[null,null,null,null,null,null,null,null,null,null,null,"        Dim itemSele As Long"]
[null,null,null,null,null,null,null,null,null,null,null,"       Dim startRow as integer"]
[null,null,null,null,null,null,null,null,null,null,null,"        LastRowA = ActiveSheet.Cells(Rows.count, \"A\").End(xlUp).row"]
[null,null,null,null,null,null,null,null,null,null,null,"        startQue = 0"]
[null,null,null,null,null,null,null,null,null,null,null,"        For itemSele = 0 To ListBox1.ListCount - 1"]
[null,null,null,null,null,null,null,null,null,null,null,"        For startRow = 1 To LastRowA"]
[null,null,null,null,null,null,null,null,null,null,null,"        If Worksheets(\"WorksheetName\").Range(\"A\" & startRow).Value = ListBox1.List(itemSele) Then"]
[null,null,null,null,null,null,null,null,null,null,null,"        ListBox1.Selected(itemSele) = True"]
[null,null,null,null,null,null,null,null,null,null,null,"        Exit For"]
[null,null,null,null,null,null,null,null,null,null,null,"        End If"]
[null,null,null,null,null,null,null,null,null,null,null,"        Next j"]
[null,null,null,null,null,null,null,null,null,null,null,"        Next"]
[null,null,null,null,null,null,null,null,null,null,null,"        End If"]

{"sheet":"Areaofobs","index":3,"n_rows":17,"n_cols":2,"rows_kept":17,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Cargo / Ballast Systems",11]
["Cert. & Docu.",2]
["Communication",6]
["Crew Management",3]
["Emgcy. Systems",13]
["Eng. / Strg. Comp.",14]
["General Appearance",15]
["Ice Opns.",17]
["ISM Related",7]
["ISPS Related",10]
["MARPOL Related",9]
["MLC Related",4]
["Mooring",12]
["Navigation",5]
["Safety / LSA / FFA",8]
["Structural Condn. / WT integrity ",16]

{"sheet":"Vessel_type","index":4,"n_rows":1,"n_cols":2,"rows_kept":1,"cut":false,"hidden":true,"merged":[]}
["Vessel_type","ID"]

{"sheet":"Deficiency_type","index":5,"n_rows":8,"n_cols":3,"rows_kept":8,"cut":false,"hidden":true,"merged":[]}
["TITLE","Type of deficiency_description","ID"]
["Breakdown",null,6]
["Critical Equipment",null,4]
["Defect",null,1]
["Guarantee Claim",null,8]
["Non Conformity",null,2]
["Observation",null,3]
["Other",null,7]

{"sheet":"VIQrefno","index":6,"n_rows":427,"n_cols":3,"rows_kept":427,"cut":false,"hidden":true,"merged":[]}
["VIQ_ref_no","Risk Value of observation","ID"]
["1.1","Low",8243]
["1.10","Low",8252]
["1.11","Low",8253]
["1.12","Low",8254]
["1.13","Low",8255]
["1.14","Low",8256]
["1.15","Low",8257]
["1.16","Low",8259]
["1.17","Low",8260]
["1.18","Low",8261]
["1.19","Low",8262]
["1.2","Low",8244]
["1.20","Low",8263]
["1.21","Low",8265]
["1.22","Low",8266]
["1.23","Low",8267]
["1.24","Low",8268]
["1.25","Low",8269]
["1.26","Low",8270]
["1.3","Low",8245]
["1.4","Low",8246]
["1.5","Low",8247]
["1.6","Low",8248]
["1.7","Low",8249]
["1.8","Low",8250]
["1.9","Low",8251]
["1.99","High",11258]
["10.1","Medium",8461]
["10.10","High",8470]
["10.11","Medium",8471]
["10.12","Very High",8472]
["10.13","Very High",8473]
["10.14","Medium",8474]
["10.15","Low",8475]
["10.16","Very High",8476]
["10.17","Very High",8477]
["10.18","High",8478]
["10.19","Very High",8479]
["10.2","Low",8462]
["10.20","High",8480]
["10.21","Medium",8481]
["10.22","Low",8482]
["10.23","Medium",8483]
["10.24","Low",8484]
["10.25","Very High",8485]
["10.26","High",8486]
["10.27","Medium",8487]
["10.28","Low",8488]
["10.29","Medium",8489]
["10.3","Medium",8463]
["10.30","High",8490]
["10.31","Very High",8491]
["10.32","Very High",8492]
["10.33","High",8493]
["10.34","High",8494]
["10.35","Very High",8495]
["10.36","Very High",8496]
["10.37","Medium",8497]
["10.38","Medium",8498]
["10.39","High",8499]
["10.4","High",8464]
["10.40","Medium",8500]
["10.41","Medium",8501]
["10.42","Medium",8502]
["10.43","Medium",8503]
["10.44","Medium",8504]
["10.45","Very High",8505]
["10.46","High",8506]
["10.47","Medium",8507]
["10.48","High",8508]
["10.49","Medium",8509]
["10.5","Low",8465]
["10.50","High",8510]
["10.51","Low",8511]
["10.52","Medium",8512]
["10.53","Medium",8513]
["10.54","High",8514]
["10.55","Low",8515]
["10.6","Very High",8466]
["10.7","Medium",8467]
["10.8","Medium",8468]
["10.9","Medium",8469]
["10.99","High",8516]
["11.1","High",8420]
["11.10","Medium",8429]
["11.11","Very High",8430]
["11.12","Low",8431]
["11.13","Low",8432]
["11.14","Medium",8433]
["11.15","Low",8434]
["11.16","Low",8435]
["11.17","Low",8436]
["11.2","Medium",8421]
["11.3","Medium",8422]
["11.4","Very High",8423]
["11.5","Medium",8424]
["11.6","Medium",8425]
["11.7","High",8426]
["11.8","Low",8427]
["11.9","Low",8428]
["11.99","High",8437]
["12.1","High",8438]
["12.10","High",8448]
["12.11","High",8449]
["12.12","High",8450]
["12.13","High",8451]
["12.14","High",8452]
["12.15","High",8453]
["12.16","High",8454]
["12.17","High",8455]
["12.18","High",8456]
["12.19","High",8457]
["12.2","High",8439]
["12.20","High",8458]
["12.21","High",8459]
["12.3","High",8441]
["12.4","High",8442]
["12.5","High",8443]
["12.6","High",8444]
["12.7","High",8445]
["12.8","High",8446]
["12.9","High",8447]
["12.99","High",8460]
["2.1","Very High",8296]
["2.1.9","Very High",11259]
["2.10","Medium",8304]
["2.11","Medium",8305]
["2.12","Low",8306]
["2.13","Low",8307]
["2.14","Low",8308]
["2.15","Low",8309]
["2.16","Medium",8310]
["2.2","Medium",8297]
["2.3","High",8295]
["2.4","Medium",8298]
["2.5","Medium",8299]
["2.6","Low",8300]
["2.7","High",8301]
["2.8","High",8302]
["2.9","Medium",8303]
["2.99","High",8311]
["3.1","High",8312]
["3.2","Very High",8313]
["3.3","High",8314]
["3.4","Low",8294]
["3.5","Medium",8315]
["3.6","High",8316]
["3.7","Very High",8317]
["3.8","Very High",8318]
["3.99","High",8319]
["4.1","High",8320]
["4.10","High",8329]
["4.11","Medium",8330]
["4.12","Very High",8331]
["4.13","Very High",8332]
["4.14","Very High",8333]
["4.15","Very High",8334]
["4.16","Very High",8335]
["4.17","Very High",8336]
["4.18","Very High",8337]
["4.19","Low",8338]
["4.2","Medium",8321]
["4.20","Very High",8339]
["4.21","High",8340]
["4.22","Low",8341]
["4.23","High",8342]
["4.24","High",8343]
["4.25","Low",8344]
["4.26","Low",8345]
["4.27","High",8346]
["4.3","Medium",8322]
["4.4","High",8323]
["4.5","Very High",8324]
["4.6","Medium",8325]
["4.7","High",8326]
["4.8","Medium",8327]
["4.9","Medium",8328]
["4.99","High",8347]
["5.1","Very High",8517]
["5.10","High",8526]
["5.11","Low",8527]
["5.12","Medium",8528]
["5.13","High",8529]
["5.14","Very High",8530]
["5.15","Medium",8531]
["5.16","Very High",8532]
["5.17","Very High",8533]
["5.18","High",8534]
["5.19","Medium",8535]
["5.2","Very High",8518]
["5.20","Medium",8536]
["5.21","Medium",8537]
["5.22","High",8539]
["5.23","Very High",8540]
["5.24","Very High",8541]
["5.25","Medium",8542]
["5.26","Medium",8543]
["5.27","Medium",8544]
["5.28","Very High",8545]
["5.29","High",8546]
["5.3","Low",8519]
["5.30","High",8547]
["5.31","High",8548]
["5.32","High",8549]
["5.33","High",8550]
["5.34","Low",8551]
["5.35","Medium",8552]
["5.36","Low",8553]
["5.37","Low",8554]
["5.38","High",8555]
["5.39","Very High",8556]
["5.4","High",8520]
["5.40","Very High",8557]
["5.41","Very High",8558]
["5.42","Medium",8559]
["5.43","High",8560]
["5.44","High",8561]
["5.45","Medium",8564]
["5.46","Medium",8565]
["5.47","Medium",8566]
["5.48","Medium",8567]
["5.5","Low",8521]
["5.6","Low",8522]
["5.7","Medium",8523]
["5.8","Medium",8524]
["5.9","Very High",8525]
["5.99","High",8568]
["6.1","Medium",8348]
["6.10","Low",8357]
["6.11","High",8358]
["6.12","Medium",8359]
["6.13","Low",8360]
["6.14","High",8361]
["6.15","High",8362]
["6.16","Very High",8363]
["6.17","Very High",8364]
["6.18","Medium",8365]
["6.19","Low",8366]
["6.2","High",8349]
["6.20","Medium",8367]
["6.21","High",8368]
["6.22","Medium",8369]
["6.3","Low",8350]
["6.4","High",8351]
["6.5","Medium",8352]
["6.6","Medium",8353]
["6.7","High",8354]
["6.8","High",8355]
["6.9","Low",8356]
["6.99","High",8370]
["7.1","High",8371]
["7.10","High",8380]
["7.11","High",8381]
["7.12","High",8382]
["7.13","Medium",8383]
["7.14","Medium",8384]
["7.15","High",8385]
["7.16","High",8386]
["7.17","High",8387]
["7.2","High",8372]
["7.3","Low",8373]
["7.4","Low",8374]
["7.5","Low",8375]
["7.6","Medium",8376]
["7.7","Low",8377]
["7.8","High",8378]
["7.9","High",8379]
["7.99","High",8388]
["8.1","Very High",8569]
["8.10","Very High",8578]
["8.100","Low",11227]
["8.101","Medium",11228]
["8.102","Low",11229]
["8.103","Low",11230]
["8.104","Low",11231]
["8.105","Medium",11232]
["8.106","Medium",11233]
["8.107","Low",11234]
["8.108","High",11235]
["8.109","Very High",11236]
["8.11","Medium",8579]
["8.110","High",11237]
["8.111","Medium",11238]
["8.112","High",11239]
["8.113","Medium",11240]
["8.114","Low",11241]
["8.115","High",11242]
["8.116","Medium",11243]
["8.117","Medium",11244]
["8.118","Medium",11245]
["8.119","High",11246]
["8.12","Medium",8580]
["8.120","High",11247]
["8.121","Medium",11248]
["8.122","High",11249]
["8.123","High",11250]
["8.124","Low",11251]
["8.125","High",11252]
["8.126","Medium",11253]
["8.127","Medium",11254]
["8.13","Medium",8581]
["8.14","Very High",8582]
["8.15","High",8583]
["8.16","Very High",8584]
["8.17","Low",8585]
["8.18","High",8586]
["8.19","High",8587]
["8.199","High",11255]
["8.2","Medium",8570]
["8.20","Medium",8588]
["8.21","High",8589]
["8.22","Very High",8590]
["8.23","Medium",8591]
["8.24","Medium",8592]
["8.25","Very High",8593]
["8.26","High",8594]
["8.27","Medium",8595]
["8.28","Medium",8596]
["8.29","High",8598]
["8.3","Very High",8571]
["8.30","High",8599]
["8.31","High",8600]
["8.32","Low",8601]
["8.33","Medium",8602]
["8.34","High",8603]
["8.35","Medium",8604]
["8.36","Medium",8605]
["8.37","High",8607]
["8.38","Medium",8608]
["8.39","Medium",8609]
["8.4","Medium",8572]
["8.40","High",8610]
["8.41","Medium",8611]
["8.42","Medium",8612]
["8.43","Very High",8613]
["8.44","High",8615]
["8.45","High",8616]
["8.46","Very High",8617]
["8.47","Very High",8618]
["8.48","Medium",8619]
["8.49","High",8620]
["8.5","Very High",8573]
["8.50","Medium",8621]
["8.51","Low",8622]
["8.52","Low",8623]
["8.53","Low",8624]
["8.54","High",8625]
["8.55","Low",11182]
["8.56","Medium",11183]
["8.57","Medium",11184]
["8.58","High",11185]
["8.59","High",11186]
["8.6","Medium",8574]
["8.60","High",11187]
["8.61","Medium",11188]
["8.62","Very High",11189]
["8.63","High",11190]
["8.64","Medium",11191]
["8.65","Low",11192]
["8.66","High",11193]
["8.67","High",11194]
["8.68","High",11195]
["8.69","Medium",11196]
["8.7","High",8575]
["8.70","Medium",11197]
["8.71","Very High",11198]
["8.72","Medium",11199]
["8.73","Medium",11200]
["8.74","High",11201]
["8.75","Medium",11202]
["8.76","Medium",11203]
["8.77","Medium",11204]
["8.78","Medium",11205]
["8.79","Medium",11206]
["8.8","Medium",8576]
["8.80","Medium",11207]
["8.81","Low",11208]
["8.82","Medium",11209]
["8.83","Low",11210]
["8.84","Low",11211]
["8.85","Medium",11212]
["8.86","Medium",11213]
["8.87","Medium",11214]
["8.88","Low",11215]
["8.89","High",11216]
["8.9","High",8577]
["8.90","High",11217]
["8.91","High",11218]
["8.92","Medium",11219]
["8.93","Low",11220]
["8.94","Low",11221]
["8.95","Medium",11222]
["8.96","Medium",11223]
["8.97","Low",11224]
["8.98","High",11225]
["8.99","Medium",11226]
["9.1","Low",8390]
["9.10","Medium",8399]
["9.11","Medium",8400]
["9.12","Medium",8401]
["9.13","Low",8402]
["9.14","Medium",8403]
["9.15","Medium",8404]
["9.16","High",8405]
["9.17","High",8406]
["9.18","Low",8407]
["9.19","Low",8408]
["9.2","Very High",8391]
["9.20","Medium",8409]
["9.21","Medium",8410]
["9.22","Low",8411]
["9.23","Low",8412]
["9.24","Medium",8413]
["9.25","Low",8414]
["9.26","Low",8415]
["9.27","Low",8416]
["9.28","Medium",8417]
["9.29","Low",8418]
["9.3","Very High",8392]
["9.4","High",8393]
["9.5","High",8394]
["9.6","Low",8395]
["9.7","Medium",8396]
["9.8","Medium",8397]
["9.9","Medium",8398]
["9.99","High",8419]

{"sheet":"Equipment_list","index":7,"n_rows":28,"n_cols":3,"rows_kept":28,"cut":false,"hidden":true,"merged":[]}
["TITLE","Equipment_list_description","ID"]
["Accommodation",null,12]
["Cargo Mach.",null,13]
["Critical Equip.",null,16]
["Deck - Machinery",null,18]
["Deck - Mooring Machinery",null,15]
["Deck - Pipe / Fittings",null,20]
["Documentation",null,21]
["E/R - Air Comp.",null,8]
["E/R - Aux. Engine",null,4]
["E/R - Aux. Mach.",null,7]
["E/R - Boiler",null,5]
["E/R - Main Engine",null,3]
["E/R - Pipes/ valves & fittings",null,9]
["E/R - Pumps",null,32]
["E/R - Purifier",null,6]
["Elect. Mach. & Equip.",null,10]
["Hull & Tanks",null,19]
["Inert Gas",null,14]
["LSA / FFA",null,17]
["Miscellaneous",null,22]
["Navigation - DGPS / EPFS / AIS",null,28]
["Navigation - ECDIS",null,25]
["Navigation - Echo Sounder / Speed Log",null,26]
["Navigation - GMDSS & Communication",null,23]
["Navigation - Others",null,11]
["Navigation - RADAR",null,24]
["Navigation - VDR / BNWAS",null,30]

{"sheet":"PSC_MOU","index":8,"n_rows":11,"n_cols":3,"rows_kept":11,"cut":false,"hidden":true,"merged":[]}
["TITLE","PSC_MOU_description","ID"]
["Asia and the Pacific",null,2]
["Caribbean",null,4]
["Europe and the North Atlantic",null,1]
["Latin America",null,3]
["The Black Sea region",null,6]
["The Indian Ocean",null,8]
["The Mediterranean",null,7]
["The Riyadh MoU",null,9]
["USCG",null,10]
["West and Central Africa",null,5]

{"sheet":"Inspection_type","index":9,"n_rows":13,"n_cols":2,"rows_kept":13,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Bunkering Audit",14]
["Cargo Audit",17]
["Engineering Audit",16]
["ISM Audit",2]
["ISPS Audit",3]
["IT Audit",10]
["MLC Audit",1]
["Mooring Audit",9]
["Nav Audit / Verification",8]
["Onboard Training",18]
["Ship Staff Insp.",15]
["Suptd. Insp.",13]

{"sheet":"Deficiency_Cause","index":10,"n_rows":8,"n_cols":3,"rows_kept":8,"cut":false,"hidden":true,"merged":[]}
["TITLE","Deficiency_Cause_description","ID"]
["Behaviour Based",null,1]
["Equipment Related",null,4]
["External Factors",null,5]
["Human Error",null,7]
["Inappropriate Procedure",null,8]
["Industry Issue",null,6]
["Knowledge Based",null,3]

{"sheet":"Observer_code","index":11,"n_rows":3,"n_cols":3,"rows_kept":3,"cut":false,"hidden":true,"merged":[]}
["TITLE","Observer_code_description","ID"]
["Owner / Marine / Tech. Suptd.",null,3]
["Ship Staff",null,2]

{"sheet":"Status_code","index":12,"n_rows":6,"n_cols":3,"rows_kept":6,"cut":false,"hidden":true,"merged":[]}
["TITLE","Status_code_description","ID"]
["Completed",null,6]
["Deferred to D D",null,5]
["In progress",null,3]
["Not Started",null,2]
["Waiting spare",null,4]

{"sheet":"PSC_ref_no","index":13,"n_rows":19,"n_cols":2,"rows_kept":19,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Alarms",9]
["Cargo operations including equipment",7]
["Certificates & Documentation",2]
["Dangerous Goods",13]
["Emergency Systems",5]
["Fire safety",8]
["ISM",16]
["ISPS",17]
["Life saving appliances",12]
["MLC, 2006",18]
["Other",19]
["Pollution Prevention",15]
["Propulsion and auxiliary machinery",14]
["Radio communication",6]
["Safety of Navigation",11]
["Structural condition",3]
["Water/Weathertight condition",4]
["Working and Living Conditions",10]

{"sheet":"Risk_value_of_obs","index":14,"n_rows":1,"n_cols":2,"rows_kept":1,"cut":false,"hidden":true,"merged":[]}
["Risk Value of observation","ID"]

{"sheet":"Year","index":15,"n_rows":18,"n_cols":1,"rows_kept":18,"cut":false,"hidden":true,"merged":[]}
["Year"]
[2014]
[2015]
[2016]
[2017]
[2018]
[2019]
[2020]
[2021]
[2022]
[2023]
[2024]
[2025]
[2026]
[2027]
[2028]
[2029]
[2030]

{"sheet":"Month","index":16,"n_rows":13,"n_cols":1,"rows_kept":13,"cut":false,"hidden":true,"merged":[]}
["Month"]
["Jan"]
["Feb"]
["Mar"]
["Apr"]
["May"]
["Jun"]
["Jul"]
["Aug"]
["Sep"]
["Oct"]
["Nov"]
["Dec"]

{"sheet":"Date_","index":17,"n_rows":32,"n_cols":1,"rows_kept":32,"cut":false,"hidden":true,"merged":[]}
["Date"]
["01"]
["02"]
["03"]
["04"]
["05"]
["06"]
["07"]
["08"]
["09"]
[10]
[11]
[12]
[13]
[14]
[15]
[16]
[17]
[18]
[19]
[20]
[21]
[22]
[23]
[24]
[25]
[26]
[27]
[28]
[29]
[30]
[31]

{"sheet":"Sheet1","index":18,"n_rows":24,"n_cols":6,"rows_kept":24,"cut":false,"hidden":true,"merged":[]}
[]
[null,"ID","E",null,"Date Recorded",1]
[null,"UNIQUE ID","F",null,"Type of Deficiency",2]
[1,"Date Recorded","G",null,"Observer code",3]
["ignore","Vessel Type","H",null,"Type of Inspection",4]
[null,"Internal / External","I",null,"Description of Deficiency",5]
[null,"Drydock","J",null,"Equipment Categories",6]
[null,"Information Sharing","K",null,"Area of Observation",7]
[null,"Critical_item","L",null,"Deficiency Cause",8]
[null,"Deficiency Type","M",null,"VIQ Ref Number",9]
[null,"Deficiency Cause","N",null,"Risk Value of Obs",10]
[null,"Inspection Type","O",null,"PSC Ref Number",11]
[null,"Equipments","P",null,"PSC MOU ID",12]
[null,"VIQ Reference Number","Q",null,"Action Taken or Required",13]
[null,"Risk Value of the observation","R",null,"Target Date",14]
[null,"PSC Reference Number","S",null,"PO Ref No.",15]
[null,"PSC MOU","T",null,"Status Code",16]
[null,"Observer Code","U",null,"Date Completed",17]
[null,"Target Date","V",null,"Drydock",18]
[null,"Status Code","W",null,"Info Sharing",19]
[null,"Description of Deficiency","X",null,"Critical Item Flag",20]
[null,"Action taken / required","Y",null,"Audit Type",21]
[null,"PO ref no","Z"]
[null,"Date completed","AA"]

{"sheet":"Ship_information","index":19,"n_rows":2,"n_cols":3,"rows_kept":2,"cut":false,"hidden":true,"merged":[]}
["Ship_ID","Ship_Name","FILE_NAME"]
["38","EAGLE (12-06-2020)","38_1606789839122.xlsm"]

{"sheet":"External_Deficiency_type","index":20,"n_rows":5,"n_cols":3,"rows_kept":5,"cut":false,"hidden":true,"merged":[]}
["TITLE","Type of deficiency_description","ID"]
["Condn of Class / Memo",null,5]
["Defect",null,1]
["Non Conformity",null,2]
["Observation",null,3]

{"sheet":"External_Inspection_type","index":21,"n_rows":11,"n_cols":2,"rows_kept":11,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Cargo Audit",17]
["Flag State Insp.",5]
["ISM Audit",2]
["ISPS Audit",3]
["MLC Audit",1]
["Nav Audit / Verification",8]
["OM Insp. (Eg. SIRE / CDI etc.)",6]
["Others (Eg. Insurance etc.)",12]
["PSC Inspection",4]
["Terminal Insp.",11]

{"sheet":"External_Observer_code","index":22,"n_rows":7,"n_cols":3,"rows_kept":7,"cut":false,"hidden":true,"merged":[]}
["TITLE","Observer_code_description","ID"]
["Class Surveyor",null,4]
["FSC Inspector",null,5]
["Others (Eg. Insurance etc.)",null,9]
["PSC Insp.",null,6]
["SIRE / CDI Insp.",null,8]
["Terminal Insp.",null,7]

{"sheet":"Sheet Version","index":23,"n_rows":2,"n_cols":2,"rows_kept":2,"cut":false,"hidden":true,"merged":[]}
["Version","Title"]
["2.0","Version 2.0"]