{"text_format":"1","workbook":"xlsx","n_sheets":24,"sheets":["Mainsheet","Completed","Calc","Areaofobs","Vessel_type","Deficiency_type","VIQrefno","Equipment_list","PSC_MOU","Inspection_type","Deficiency_Cause","Observer_code","Status_code","PSC_ref_no","Risk_value_of_obs","Year","Month","Date_","Sheet1","Ship_information","External_Deficiency_type","External_Inspection_type","External_Observer_code","Sheet Version"],"not_rendered":{"charts":0,"images":5,"macros":1,"external_links":0,"defined_names":12,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Mainsheet","index":0,"n_rows":53,"n_cols":28,"rows_kept":53,"cut":false,"hidden":false,"merged":[[10,8,10,9],[10,12,10,13],[12,6,12,27],[8,6,8,27]]}
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,"Defect - Damage Monitoring Sheet"]
[]
[null,null,null,null,null,null,null,"Date of Report","31-Aug-2020",null,null,"Ship Name","ATHERINA (29-07-2020)"]
[]
[null,null,null,null,null,null,"VERSION : 2.0"]
[]
[]
[]
[null,null,null,null,"ID","UNIQUE ID","Date Recorded","Type of Deficiency","Observer code","Type of Inspection","Description of Deficiency","Equipment Categories","Area of Observation","Deficiency Cause","VIQ Ref Number","Risk Value of Obs","PSC Ref Number","PSC MOU ID","Action Taken or Required","Target Date","PO Ref No.","Status Code","Date Completed","Drydock","Info Sharing","Critical Item","Audit Type","Superintendent Remarks"]
[null,null,null,null,11179,"83_5 Apr 2020 13:41:54","2019-03-25","Defect","Ship Staff","Ship Staff Insp.","Composite boiler back firing occasionally, furnace space and smoke tubes water washed with high pressure as we saw lot of unburnt HFO in furnace and tubes. Air and fuel to adjust as steam pressure not coping up.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Kangrim service engineer attended the vessel at Singapore on 22nd April'19 and suggested that the tubes require chemical cleaning .This is reason for blowback due to high back pressure.","2020-07-30","","Not Started",null,"No","No","No","Internal"]
[null,null,null,null,11181,"83_5/4/2020 5:54:41 PM","2019-04-10","Defect","Owner / Marine / Tech. Suptd.","Ship Staff Insp.","ME Exhuast valve rail valve timing reaching 1.5ms. Will require replacement in due course","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","ME performance taken, as of now rail valve timings are below 1.5ms. Requisition raised.","2020-07-10","","Waiting spare",null,"No","No","No","Internal"]
[null,null,null,null,11187,"83_5 Apr 2020 14:17:45","2019-10-10","Defect","Ship Staff","Ship Staff Insp.","HFO purifer No-2 Bowl is not opening when purifier open up for overhaul.","E/R - Purifier","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Work in progress, But eventually bowl need to send to workshop to open lock ring on purifer bowl.","2020-07-15","","In progress",null,"No","No","No","Internal"]
[null,null,null,null,11198,"83_6/4/2020 6:45:10 AM","2020-04-05","Defect","Ship Staff","Ship Staff Insp.","No. 1 Electric Cargo Pump VFD attended by Danfoss technician however same not operational due to burnt Measurement PCB.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.25","Very High","","","Service engioneers attendance is required","2020-07-05","","In progress",null,"No","No","No","Internal"]
[null,null,null,null,11201,"83_6/4/2020 6:51:06 AM","2020-04-05","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","M4, M5 and M7 Mooring winch speed control valve 4/3 hydraulic block needs to be replaced. Spares required for the same. The condition of few other blocks is also not good and will need to be replaced. ","Deck - Mooring Machinery","Mooring","Equipment Related",9.17,"High","Not Applicable","Not Applicable","To request for Hydraulic blocks","2020-07-05",null,"Not Started",null,"No","No","No","Internal"]
[null,null,null,null,11203,"83_6/4/2020 6:56:34 AM","2020-04-05","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ME torsional vibrational damper ( Geslinger ) in ECR not working and alarm active. Power switched ON but need more investigation.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Need to request for spare","2020-07-05","","Not Started",null,"No","No","No","Internal"]
[null,null,null,null,11204,"83_6/4/2020 7:00:08 AM","2020-04-05","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Aconis GCE module will require upgrade in due course once starts failing.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.23","Medium","","","Need to request","2020-07-04","","Not Started",null,"No","No","No","Internal"]
[null,null,null,null,11205,"83_6/4/2020 7:05:55 AM","2020-04-05","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","No centrifugal Lubeoil filter on DG's","E/R - Aux. Engine","Emgcy. Systems","Equipment Related","10.32","Very High","","","Need to request ","2020-07-05","","Not Started",null,"No","No","No","Internal"]
[null,null,null,null,11207,"83_6/4/2020 7:10:16 AM","2020-04-05","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","IG additional O2 panel installation (MESQAC requirement)","Inert Gas","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Fitted but not working, reminders were sent but no response","2020-07-05","","Deferred to D D",null,"No","No","No","Internal"]
[null,null,null,null,11208,"83_6/4/2020 7:12:13 AM","2020-04-05","Non Conformity","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Many Operational and Critical Spares noted missing on board and are required to be ordered and placed on board.","Critical Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Requisitions raised, awaiting for supply","2020-07-05","","Waiting spare",null,"No","No","No","Internal"]
[null,null,null,null,11209,"83_6/4/2020 7:17:35 AM","2020-04-05","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Migration to LED Lighting","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.23","Medium","","","Inprogress","2020-07-05","","In progress",null,"No","No","No","Internal"]
[null,null,null,null,11210,"83_6/4/2020 7:20:26 AM","2020-04-05","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","welding curtain for workshop welding area to renew","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Requisition raised ATHE200034","2020-07-05","ATHE200034","Waiting spare",null,"No","No","No","Internal"]
[null,null,null,null,11211,"83_6/4/2020 7:22:46 AM","2020-04-05","Critical Equipment","Owner / Marine / Tech. Suptd.","Suptd. Insp.","DG govenor, air starter and turbo chrager - not spare onboard","Critical Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Request made, to be supplied by owners","2020-07-05","","Waiting spare",null,"No","No","No","Internal"]
[null,null,null,null,11212,"83_6/4/2020 7:03:37 AM","2020-04-05","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Himsen DG's will require 2020 modification in due course.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Requisition raised ATHE190139","2020-07-05","ATHE190139","Waiting spare",null,"No","No","No","Internal"]
[null,null,null,null,12106,"83_3 May 2020 16:57:22","2020-04-30","Observation","Ship Staff","Ship Staff Insp.","NO. 2 COP AUS SEPERATOR LEVEL SHOWING INCORRECT READING.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.8","Medium","","","Diaphram of transmiter found broken beyond repair. Requisition to be made for new transmitter.","2020-07-15","","Not Started",null,"No","No","No","Internal"]
[null,null,null,null,13220,"83_11-Jun-20 16:20:55","2020-05-15","Defect","Ship Staff","Ship Staff Insp.","Bridge Control Console  stbd side \"Console  power, Fire pump's & Alarm lamps dimmer switch not working.","Navigation - Others","Navigation","Equipment Related","4.7","High","","","XXXXXX","2020-08-31","","Not Started",null,"No","No","No","Internal"]
[null,null,null,null,13221,"83_11-Jun-20 16:32:15","2020-06-03","Defect","Ship Staff","Ship Staff Insp.","A-deck officer duty mess room clock not working","Accommodation","General Appearance","Equipment Related","","","","","XXXXXX","2020-08-25","","Not Started",null,"No","No","No","Internal"]
[null,null,null,null,13227,"83_1/7/2020 06:54:54","2020-07-01","Observation","Ship Staff","Ship Staff Insp.","GALLEY OVEN IS GIVING LOW INSULATION ALARM NEED TO REPLACE HEATING ELEMENT","Elect. Mach. & Equip.","Crew Management","Equipment Related",10.31,"Very High","Not Applicable","Not Applicable","REQUISITION RAISED AWAITING SPARES","2020-07-28","ATHE200156","Waiting spare",null,"No","No","No","Internal"]
[null,null,null,null,null,"83_2/9/2020 6:45:13 PM","2020-08-25","Observation","Ship Staff","Ship Staff Insp.","Mooring Winch M1 is operating at low speed compared to other winches.","Deck - Mooring Machinery","Mooring","Equipment Related",9.14,"Medium","Not Applicable","Not Applicable","Speed adjustment carried out, also the speed change block swapped from other winch. No change in speed observed.","2020-11-25",null,"In progress",null,"No",null,null,"Internal"]
[null,null,null,null,null,"83_2/9/2020 7:00:09 PM","2020-08-30","Defect","Ship Staff","Ship Staff Insp.","# 1 D/G winding T & S thermistors & # 2 D/G winding S thermistor are malfunctioning","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Awaiting for office suggestion ","2020-11-30",null,"In progress",null,"No",null,null,"Internal"]
[null,null,null,null,null,"83_24 Sep 2020 16:51:02","2020-09-16","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Galley dish washer is not operational.","Miscellaneous","General Appearance","Behaviour Based",null,null,"Not Applicable","Not Applicable","To check and rectify","2020-10-16",null,"Not Started",null,"No",null,null,"Internal"]
[null,null,null,null,null,"83_24 Sep 2020 16:52:55","2020-09-16","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Vinyl flooring in officer's and crew mess room is dirty.","Accommodation","General Appearance","Behaviour Based",null,null,"Not Applicable","Not Applicable","Stipping and waxing to be carried out.","2020-10-16",null,"In progress",null,"No",null,null,"Internal"]
[null,null,null,null,null,"83_24 Sep 2020 18:18:44","2020-09-16","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Fittings (for support pipelines) port manifold rusted and needs immediate maintenance.","Deck - Pipe / Fittings","General Appearance","Human Error",null,null,"Not Applicable","Not Applicable","Derusting and painting to be carried out.","2020-10-15",null,"In progress",null,"No",null,null,"Internal"]
[null,null,null,null,null,"83_24/9/2020 23:17:40","2020-09-16","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Accommodation is around 28 deg C. The AC compressor is to be checked for proper functioning.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Waiting for spare","2020-10-10",null,"Not Started",null,"No",null,null,"Internal"]
[null,null,null,null,null,"83_24/9/2020 23:21:02","2020-09-16","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","GE#3 OMD is isolated. This is to be investigated.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Received PCB is wrong supply.","2020-10-10",null,"In progress",null,"No",null,null,"Internal"]
[null,null,null,null,null,"83_23 Nov 2020 19:02:27","2020-11-23","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Many areas on main deck noted with top coat paint eroding and base layer visible, same to be recoated with full coat.","Miscellaneous","General Appearance","External Factors",null,null,"Not Applicable","Not Applicable","Affected areas to be derusted, cleaned with fresh water and then recoat by spray machine.","2021-04-15",null,"In progress",null,"No",null,null,"Internal"]
[null,null,null,null,null,"83_23 Nov 2020 19:12:17","2020-11-23","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Aft scupper above draft mark to be inserted with a extention so that the drain water does not affect the aft draft marks","Miscellaneous","General Appearance","External Factors",null,null,"Not Applicable","Not Applicable","Extension to be made and fitted in aft scupper above draft marks.","2021-01-15",null,"Not Started",null,"No",null,null,"Internal"]
[null,null,null,null,null,"83_23 Nov 2020 19:17:48","2020-11-23","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Life boat Davit Support Pillar is to be painted. ","Miscellaneous","General Appearance","External Factors",null,null,"Not Applicable","Not Applicable","To be painted","2020-12-21",null,"Not Started",null,"No",null,null,"Internal"]
[null,null,null,null,null,"83_24/11/2020 14:18:56","2020-11-23","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Main switchboard 220 V earth fault light for S and T phase not lit.Reading is 0.6 ohm","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related",10.38,"Medium","Not Applicable","Not Applicable","Req.raised ","2021-01-30","ATHE 200270","Waiting spare",null,"No",null,null,"Internal"]
[null,null,null,null,null,"83_24/11/2020 18:40:34","2020-11-23","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ME unit 2,4,6,7 to overhaul","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Unit 2 completed","2021-01-30",null,"In progress",null,"No",null,null,"Internal"]
[null,null,null,null,null,"83_24/11/2020 18:45:04","2020-11-23","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","VFD ACB not fully operational","Cargo Mach.","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","OFFlanded for service ashore","2020-12-30",null,"Not Started",null,"No",null,null,"Internal"]
[null,null,null,null,null,"83_24-Nov-20 19:21:57","2020-11-23","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Forward whistle noted inoperational during the inspection. Same to be checked and rectified.","Navigation - Others","Navigation","Equipment Related",null,null,"Not Applicable","Not Applicable","Forward whistle repaired and made operational temporarily, vessel awaiting spares for the same.","2021-01-15","ATHE200278","In progress",null,"No",null,null,"Internal"]
[null,null,null,null,null,"83_28/11/2020 14:01:31","2020-11-23","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Composite boiler to try out to see effectiveness of cleaning","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","To try out.","2020-12-10",null,"In progress",null,"No",null,null,"Internal"]
[null,null,null,null,null,"83_28/11/2020 14:58:56","2020-11-28","Observation","Ship Staff","Ship Staff Insp.","AE#1 Turbocharger speed sensor not working","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Spare sensor ordered.","2021-01-31","ATHE200280","Waiting spare",null,"No",null,null,"Internal"]
[null,null,null,null,null,"83_19/12/2020 21:50:34","2020-12-10","Breakdown","Ship Staff","Ship Staff Insp.","OWS Electric heater not operational due to hole in the sensing tube.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related",10.31,"Very High","Not Applicable","Not Applicable","Requisition raised.","2021-01-05","REQ.No:ATHE 200286","Waiting spare",null,"No",null,null,"Internal"]
[null,null,null,null,null,"83_22/12/2020 2:18:51 AM","2020-12-19","Defect","Ship Staff","Ship Staff Insp.","Forward whistle is not operational","Navigation - Others","Navigation","Equipment Related",null,null,"Not Applicable","Not Applicable","REQUIRE SPOARES ","2021-01-04",null,"Waiting spare",null,"No",null,null,"Internal"]

{"sheet":"Completed","index":1,"n_rows":361,"n_cols":28,"rows_kept":361,"cut":false,"hidden":false,"merged":[[10,8,10,9],[10,12,10,13],[12,6,12,27],[8,6,8,27]]}
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,"Defect - Damage Monitoring Sheet"]
[]
[null,null,null,null,null,null,null,"Date of Report","31-Aug-2020",null,null,"Ship Name","ATHERINA (29-07-2020)"]
[]
[null,null,null,null,null,null,"VERSION : 2.0"]
[]
[]
[]
[null,null,null,null,"ID","UNIQUE ID","Date Recorded","Type of Deficiency","Observer code","Type of Inspection","Description of Deficiency","Equipment Categories","Area of Observation","Deficiency Cause","VIQ Ref Number","Risk Value of Obs","PSC Ref Number","PSC MOU ID","Action Taken or Required","Target Date","PO Ref No.","Status Code","Date Completed","Drydock","Info Sharing","Critical Item","Audit Type","Superintendent Remarks"]
[null,null,null,null,10136,"83_21/1/2020 11:06:47 PM","2018-09-16","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","All overboard valves in Engine room to be operated manually and hydraulic pump where fitted.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.31","Very High","","","Done","2019-09-30","","Completed","2019-09-20","No","No","No","Internal","Ensure this is done on regular basis."]
[null,null,null,null,8412,"83_Tue Dec 10 2019 03:44:30 GMT+0000 (Coordinated Universal Time)","2019-03-08","Defect","Ship Staff","Ship Staff Insp.","OWS ist stage filter fully wasted/oil soaked","Critical Equip.","Eng. / Strg. Comp.","Equipment Related","6.17","Very High","","","First stage filter replaced with the spare one.","2019-04-30","","Completed","2019-04-24","No","No","No","Internal"]
[null,null,null,null,2200,"83_14/10/2019 6:49:34 PM","2019-03-10","Defect","Ship Staff","Ship Staff Insp.","Engine room crane wire needs  renewal.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.28","Low","","","Wire renewed on 7th Apr 2019, job completed.","2019-06-20","","Completed","2019-04-07","No","No","No","Internal"]
[null,null,null,null,2202,"83_14/10/2019 6:52:48 PM","2019-03-13","Defect","Ship Staff","Ship Staff Insp.","Sewage holding tank level gauge inoperative .","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Gauge renewed.","2019-07-30","","Completed","2019-06-09","No","No","No","Internal"]
[null,null,null,null,8400,"83_Sun Nov 10 2019 01:56:41 GMT+0000 (Coordinated Universal Time)","2019-03-17","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","WECS computer for wartisila need to upgrade.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Upgraded with new software and hardware.","2019-04-25","","Completed","2019-04-23","No","No","No","Internal"]
[null,null,null,null,2122,"83_2019-10-10 20:35:16.000","2019-03-20","Defect","Ship Staff","Ship Staff Insp.","Aconis AMS monitor in ECR console are not original and fitted with normal PC monitor.\t","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Original monitor ordered and fixed","2019-04-30","ATHE195060","Completed","2019-04-24","No","No","No","Internal"]
[null,null,null,null,2145,"83_2019-12-10 03:46:20.000","2019-03-20","Defect","Ship Staff","Ship Staff Insp.","Fire bilge and GS pump No.1 Mechanical seal leaking.","LSA / FFA","Eng. / Strg. Comp.","Equipment Related","5.38","High","","","Mech.seal replaced with the spare one.","2019-04-30","","Completed","2019-04-25","No","No","No","Internal"]
[null,null,null,null,2150,"83_2019-12-10 03:55:40.000","2019-03-20","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Graviner oil mist detector EPROM and software upgrade.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.21","Medium","","","monitoring and no issues till now. ","2019-05-30","","Completed","2019-04-26","No","No","No","Internal"]
[null,null,null,null,2133,"83_2019-11-10 01:58:31.999","2019-03-21","Defect","Ship Staff","Ship Staff Insp.","Engine performance system for AE and ME","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","ME and DG performance taken.","2019-04-26","","Completed","2019-04-26","No","No","No","Internal"]
[null,null,null,null,2205,"83_14/10/2019 7:00:30 PM","2019-03-23","Defect","Ship Staff","Ship Staff Insp.","DG3 Air starting reducing valve malfunctioning.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Reducing valve o'hauled and operating satisfactory .","2019-06-25","","Completed","2019-06-10","No","No","No","Internal"]
[null,null,null,null,2240,"83_15/10/2019 11:10:03 AM","2019-03-26","Defect","Ship Staff","Ship Staff Insp.","Many Pressure gauges faulty in ER need to be replaced.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Supplied at yard and replaced . Will identify more and replace pending in due course.","2019-09-25","","Completed","2019-08-15","No","No","No","Internal"]
[null,null,null,null,2182,"83_14/10/2019 6:06:05 PM","2019-03-27","Defect","Ship Staff","Ship Staff Insp.","Observation tank level gauge glass found to be broken at the top side.\t","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.25","Very High","","","Gauge glass renewed","2019-06-01","","Completed","2019-05-21","No","No","No","Internal"]
[null,null,null,null,8403,"83_Sun Nov 10 2019 14:52:04 GMT+0000 (Coordinated Universal Time)","2019-03-28","Defect","Ship Staff","Ship Staff Insp.","IG additional O2 panel installation ( MESQAC requirement)","Inert Gas","Eng. / Strg. Comp.","Equipment Related","8.22","Very High","","","New O2 panel installed with all the fittings.","2019-04-25","","Completed","2019-04-18","No","No","No","Internal"]
[null,null,null,null,2125,"83_2019-11-10 01:36:16.000","2019-03-30","Defect","Ship Staff","Ship Staff Insp.","Dust in many electric panels. Many contacts causing low insulation alarm. To clean them and order spares contacts.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.37","Medium","","","MSBD and AMS panel cleaning carried out at yard. Spare contactors ordered.","2019-04-10","ATHE195030","Completed","2019-04-04","No","No","No","Internal"]
[null,null,null,null,2128,"83_2019-11-10 01:46:10.000","2019-03-30","Defect","Ship Staff","Ship Staff Insp.","Hydraulic top bracing FWD leaking when charging oil. Suspect cylinder seal damaged and require replacement.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Gas changed in accumulator. As off now no leak is observed and have 1set of seals as spares.","2019-05-30","","Completed","2019-04-25","No","No","No","Internal"]
[null,null,null,null,2130,"83_2019-11-10 01:51:39.000","2019-03-30","Defect","Ship Staff","Ship Staff Insp.","DG No.3 exhaust gas temp A sensor to be replaced.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Sensor replaced with spare new sensor.","2019-04-25","","Completed","2019-04-25","No","No","No","Internal"]
[null,null,null,null,2148,"83_2019-12-10 03:52:13.000","2019-03-30","Defect","Ship Staff","Ship Staff Insp.","IG scrubber high level float alarm erratic and temporarily repaired.","Inert Gas","Eng. / Strg. Comp.","Equipment Related","8.25","Very High","","","High level float renewed and tried out-satisfactory.","2019-04-30","","Completed","2019-04-26","No","No","No","Internal"]
[null,null,null,null,8396,"83_Sun Nov 10 2019 01:46:10 GMT+0000 (Coordinated Universal Time)","2019-03-30","Defect","Ship Staff","Ship Staff Insp.","Hydraulic top bracing FWD leaking when charging oil. Suspect cylinder seal damaged and require replacement.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Gas changed in accumulator. As off now no leak is observed and have 1set of seals as spares.","2019-05-30","","Completed","2019-04-25","No","No","No","Internal"]
[null,null,null,null,2189,"83_14/10/2019 6:19:38 PM","2019-04-01","Defect","Ship Staff","Ship Staff Insp.","DG 3 LO priming pp motor making noise. Require replacement. Spare motor onboard.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Pump and motor decoupled,inspected.Motor o'hauled and tried out-satisfactory.","2019-06-30","","Completed","2019-05-25","No","No","No","Internal"]
[null,null,null,null,2191,"83_14/10/2019 6:22:08 PM","2019-04-01","Defect","Ship Staff","Ship Staff Insp.","Galley out of 4 plates 2 are working normal.","Elect. Mach. & Equip.","General Appearance","Equipment Related","10.37","Medium","","","2 no.hot plates renewed and working satisfactory.","2019-07-01","","Completed","2019-05-30","No","No","No","Internal"]
[null,null,null,null,2235,"83_15/10/2019 11:01:40 AM","2019-04-01","Defect","Ship Staff","Ship Staff Insp.","Main Engine Various operational and critical spares need to placed on board eg. ICU, RPME, Crank angle sensor, drain valve etc.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.13","Very High","","","Spares ordered and received in full.","2019-07-01","ATHE195022","Completed","2019-07-20","No","No","No","Internal"]
[null,null,null,null,2244,"83_15/10/2019 11:15:26 AM","2019-04-01","Defect","Ship Staff","Ship Staff Insp.","220 volt alarm at many places. Need to replace light bulbs, fititng at many palces.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.38","Medium","","","Many places rectified in acomodation and lighting and still in progress. Will require to roder light fittings and consumables.","2019-09-30","","Completed","2019-08-30","No","No","No","Internal"]
[null,null,null,null,11213,"83_05-Apr-20 02:20:36","2019-04-01","Defect","Ship Staff","Ship Staff Insp.","Deck seal flow sensor bypassed.","Inert Gas","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","FLOW RELAY REPLACED WITH SPARE RECEIVED AT SUEZ.","2019-11-15","ATHE190159","Completed","2020-02-07","No","No","No","Internal"]
[null,null,null,null,2258,"83_17/10/2019 6:37:49 PM","2019-04-01","Defect","Ship Staff","Ship Staff Insp.","Galley oven giving low insulation.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.38","Medium","","","Spare heating element and thermostat controller receive but it is defective as it gives low insulation.Office has been informed.","2019-09-30","ATHE190115\t","Completed","2019-10-05","No","No","No","Internal"]
[null,null,null,null,2097,"83_16/10/2019 6:26:56 PM","2019-04-02","Defect","Ship Staff","Ship Staff Insp.","Main engine servo leak drive rail unit alarm sensor to replace (Infront of ECR).\t\t\t","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Spare received.same renewed. working satisfactory.","2019-09-30","","Completed","2020-01-16","No","No","No","Internal"]
[null,null,null,null,2127,"83_2019-11-10 01:41:57.999","2019-04-02","Defect","Ship Staff","Ship Staff Insp.","Residual BN and Iron to measure and OBSERVE the liner surface. LO test kit to order.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.7","Medium","","","Test kit received and samples send for shore analysis. Onboard test to be carried out shortly.","2019-04-29","","Completed","2019-04-29","No","No","No","Internal"]
[null,null,null,null,2139,"83_2019-10-11 15:05:18.000","2019-04-02","Defect","Ship Staff","Ship Staff Insp.","Blue line bulkhead master valve suspect passing.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.11","Medium","","","RO received, Job completed.","2019-04-15","ATHE195057","Completed","2019-04-12","No","No","No","Internal"]
[null,null,null,null,2152,"83_2019-10-12 04:00:27.999","2019-04-02","Defect","Ship Staff","Ship Staff Insp.","4C COT Stripper valve passing.","Deck - Machinery","Cargo / Ballast Systems","Equipment Related","8.11","Medium","","","Seat ring  renewed","2019-04-16","ATHE195057","Completed","2019-04-16","No","No","No","Internal"]
[null,null,null,null,2155,"83_2019-12-10 06:14:42.000","2019-04-02","Defect","Ship Staff","Ship Staff Insp.","Cargo and Bunker Overfill alarm hooters on deck not working. ","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","8.14","Very High","","","RO Raised, spares received at Canaport, deck overfill alarm hooters working, bunker overfill alarm hooter remains ATHE190089.","2019-04-22","ATHE190033 & ATHE190089","Completed","2019-04-22","No","No","No","Internal"]
[null,null,null,null,2156,"83_2019-12-10 06:17:20.000","2019-04-02","Defect","Ship Staff","Ship Staff Insp.","Both pilot ladders not solas approved.\t\t","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.47","Medium","","","RO RECEIVED,  NEW PILOT LADDER  RECEIVED & IN USE.","2019-04-22","ATHE195079","Completed","2019-04-22","No","No","No","Internal"]
[null,null,null,null,2157,"83_2019-12-10 06:19:04.999","2019-04-02","Defect","Ship Staff","Ship Staff Insp.","6 Nos Mandal shackle need renewal, Found wasted.","Deck - Machinery","General Appearance","Equipment Related","9.17","High","","","NEW MANDAL SHACKLE RECEIVED & RENEWED.","2019-04-22","ATHE190031","Completed","2019-04-22","No","No","No","Internal"]
[null,null,null,null,2162,"83_2019-12-10 06:32:24.000","2019-04-02","Defect","Ship Staff","Ship Staff Insp.","Slop s COT Valve passing.","Deck - Machinery","Cargo / Ballast Systems","Equipment Related","8.11","Medium","","","Seat ring renewed.","2019-04-28","ATHE195057","Completed","2019-04-30","No","No","No","Internal"]
[null,null,null,null,2166,"83_2019-12-10 06:39:06.000","2019-04-02","Defect","Ship Staff","Ship Staff Insp.","VECS System pressure guage not working in CCR.","Elect. Mach. & Equip.","Emgcy. Systems","Equipment Related","8.25","Very High","","","This was due to wrong connections given in shipyard,same rectified.","2019-05-10","","Completed","2019-05-07","No","No","No","Internal"]
[null,null,null,null,2169,"83_2019-12-10 06:44:50.000","2019-04-02","Defect","Ship Staff","Ship Staff Insp.","2P WBT Main valve passing.","Deck - Pipe / Fittings","General Appearance","Equipment Related","8.11","Medium","","","Valve seat ring renewed.","2019-05-13","","Completed","2019-05-11","No","No","No","Internal"]
[null,null,null,null,2176,"83_2019-12-10 06:57:18.000","2019-04-02","Defect","Ship Staff","Ship Staff Insp.","SEVERAL WHEELS FOR COW MACHINE VALVE & FIRE LINE FOUND BROKEN & DAMAGED.\t\t","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.11","Medium","","","All renewed","2019-05-20","","Completed","2019-05-18","No","No","No","Internal"]
[null,null,null,null,2181,"83_14/10/2019 6:04:31 PM","2019-04-02","Defect","Ship Staff","Ship Staff Insp.","AC controller fluctiaing and suspect PCB will fail in due course. Other PCB already renenwed recently.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Spare PCB ordered and received on board, kept as spare . Old PCB working satisfactory after cleaning PCB and wiring connections retighten.","2019-07-10","","Completed","2019-05-21","No","No","No","Internal"]
[null,null,null,null,2188,"83_14/10/2019 6:18:11 PM","2019-04-02","Defect","Ship Staff","Ship Staff Insp.","Air conditon plant solenoid valve for compressor oil return malfunction.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Solenoid valve replaced.","2019-07-01","","Completed","2019-05-24","No","No","No","Internal"]
[null,null,null,null,2136,"83_2019-11-10 14:54:31.000","2019-04-03","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Boiler and Composite boilers need service engineers to check the settings for IG and water level controllers.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Kangrim service Engineers attended at singapore. Both Aux. boilers are operating satisfactory.","2019-04-25","","Completed","2019-04-22","No","No","No","Internal"]
[null,null,null,null,2185,"83_14/10/2019 6:11:48 PM","2019-04-03","Defect","Ship Staff","Ship Staff Insp.","Pressure transmitter (oil and suction)  of AC 2 plant temporarily repaired.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","It is working ok .Will replace as required.","2019-07-10","","Completed","2019-05-22","No","No","No","Internal"]
[null,null,null,null,2241,"83_15/10/2019 11:11:28 AM","2019-04-03","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Soot collecting tank to fabricate for collecting / separating soot.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","To be done in due course of time","2021-07-02","","Completed","2019-08-15","No","No","No","Internal","Ensure same is entered in REFMAN."]
[null,null,null,null,11180,"83_5 Apr 2020 14:02:38","2019-04-05","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Servo pump pressure drops very fast after stopping Main engine. Need to investigate the reason and repair.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","As per Wartsila Service Engineers mail dated 22 Jun 2020, the immediate drop in servo oil pressure after stopping the ME is normal. Hence this defect is considered as closed","2020-07-30","","Completed","2020-06-22","No","No","No","Internal"]
[null,null,null,null,8402,"83_Sun Nov 10 2019 14:49:52 GMT+0000 (Coordinated Universal Time)","2019-04-05","Defect","Ship Staff","Ship Staff Insp.","Damaged and Oil soaked lagging to be replaced in some loacations in the Engine room.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.19","Very High","","","All damaged laggings replaced with spare laggings.","2019-04-25","","Completed","2019-04-25","No","No","No","Internal"]
[null,null,null,null,8406,"83_Sun Nov 10 2019 15:02:49 GMT+0000 (Coordinated Universal Time)","2019-04-05","Defect","Ship Staff","Ship Staff Insp.","Hot water calorifier steam heater body gasket leaking.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Gasket renewed. No leaks in the system.","2019-04-10","","Completed","2019-04-05","No","No","No","Internal"]
[null,null,null,null,8417,"83_Tue Dec 10 2019 03:53:58 GMT+0000 (Coordinated Universal Time)","2019-04-05","Defect","Ship Staff","Ship Staff Insp.","Incinerator refractory to order. Sludge burning to start in incinrateor.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Refractory is in good condition. Sludge burning started in incinerator.","2019-04-28","","Completed","2019-04-26","No","No","No","Internal"]
[null,null,null,null,2137,"83_2019-11-10 14:56:41.000","2019-04-07","Defect","Ship Staff","Ship Staff Insp.","Emergency generator cooling water pressure switch bypassed.","Elect. Mach. & Equip.","Emgcy. Systems","Equipment Related","10.32","Very High","","","Pressure switch renewed.","2019-04-25","","Completed","2019-04-24","No","No","No","Internal"]
[null,null,null,null,8399,"83_Sun Nov 10 2019 01:54:46 GMT+0000 (Coordinated Universal Time)","2019-04-08","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","No recovery unit / pump - bottles for Main ac for collecting gas.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Received at call singapore","2019-04-25","","Completed","2019-04-23","No","No","No","Internal"]
[null,null,null,null,2124,"83_2019-10-11 01:33:07.000","2019-04-09","Defect","Ship Staff","Ship Staff Insp.","ME fuel oil fine filter change over mechanism hard.\t","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Change over mechanism overhauled and now its working satisfactory.","2019-04-15","","Completed","2019-04-10","No","No","No","Internal"]
[null,null,null,null,2123,"83_2019-11-10 01:29:21.000","2019-04-10","Defect","Ship Staff","Ship Staff Insp.","Steering gear No 1 pp having oil leak from pp block. Need to check leak location.\t\t","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.39","High","","","Pump casing block tightened and found no leak on the pump side.","2019-04-30","","Completed","2019-04-24","No","No","No","Internal"]
[null,null,null,null,2140,"83_2019-11-10 15:12:40.000","2019-04-10","Defect","Ship Staff","Ship Staff Insp.","440 Volt alarm due to low insulation from ER vent fan and Boiler no:1 panel. Need investigation.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.38","Medium","","","Boiler No:1 faulty contactor replaced and ER vent fan naked wire insulated. 440V insulation meter shows now infinity.","2019-04-13","","Completed","2019-04-11","No","No","No","Internal"]
[null,null,null,null,2171,"83_2019-12-10 06:48:52.000","2019-04-10","Defect","Ship Staff","Ship Staff Insp.","Stbd windlass Hyd cylinder for engaing / disengaging gear is not working.","Deck - Mooring Machinery","Mooring","Equipment Related","9.2","Very High","","","Hyd.cylinder eased up and found to working satisfactory.","2019-07-08","","Completed","2019-05-14","No","No","No","Internal"]
[null,null,null,null,2177,"83_14/10/2019 5:54:41 PM","2019-04-10","Defect","Ship Staff","Ship Staff Insp.","No.2 COP Discharge NRV (750 A) leaking from flange. Gasket for same needs to be replaced.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.11","Medium","","","Gasket need to be renewed , flange need to be tighten.","2019-05-18","","Completed","2019-05-16","No","No","No","Internal"]
[null,null,null,null,2209,"83_15/10/2019 10:25:26 AM","2019-04-10","Defect","Ship Staff","Ship Staff Insp.","Alarm monitoring system diode defective.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.37","Medium","","","Diode renewed.","2019-06-30","","Completed","2019-06-11","No","No","No","Internal"]
[null,null,null,null,2096,"83_16/10/2019 6:25:12 PM","2019-04-12","Defect","Ship Staff","Ship Staff Insp.","No.1 IG blower main valve getting stuck while opening and requires repair kit and to be overhauled.","Inert Gas","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","New actuator fitted and calibrated and tried out.Found satisfactory. ","2019-09-30","","Completed","2019-12-02","No","No","No","Internal"]
[null,null,null,null,2098,"83_16/10/2019 6:28:39 PM","2019-04-12","Defect","Ship Staff","Ship Staff Insp.","Ballast remote sounding guages for all tanks showing erratic readings except 1P ","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.8","Medium","","","Ballast tanks purge heads dismantled, overhauled,cleaned & cleared. Two purge unit  requisitioned raised. Will check the trueness of readings  during discharging opeartion.","2019-11-15","ATHE195089\t","Completed","2019-12-30","No","No","No","Internal"]
[null,null,null,null,2126,"83_2019-11-10 01:38:36.000","2019-04-12","Defect","Ship Staff","Ship Staff Insp.","IG panel turn switch malfuntion. Presently wire disconnected.","Inert Gas","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Switch repaired and its function check carried out.","2019-04-15","","Completed","2019-04-14","No","No","No","Internal"]
[null,null,null,null,2129,"83_2019-11-10 01:49:41.999","2019-04-12","Defect","Ship Staff","Ship Staff Insp.","ME lub oil sump to top up with 6000 litres of oil as presently level around 36,000 ltr.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Sump oil topped up with 6500 litres.","2019-04-15","","Completed","2019-04-13","No","No","No","Internal"]
[null,null,null,null,2147,"83_2019-12-10 03:49:10.000","2019-04-12","Defect","Ship Staff","Ship Staff Insp.","DG 2 fuel filter leaking oil from top.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.19","Very High","","","Leakage rectified.","2019-04-30","","Completed","2019-04-26","No","No","No","Internal"]
[null,null,null,null,2151,"83_2019-12-10 03:58:05.999","2019-04-12","Defect","Ship Staff","Ship Staff Insp.","Inert gas temp found to be going higher withing short period of operation.","Inert Gas","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Scruuber tower all nozzles removed and cleared off dirt/sea shells.","2019-05-30","","Completed","2019-04-26","No","No","No","Internal"]
[null,null,null,null,2153,"83_2019-12-10 05:02:49.999","2019-04-12","Defect","Ship Staff","Ship Staff Insp.","Kongsberg System Max. depths for all centre tanks needs to be corrected  noted a difference in the Max. depths in the sounding tables and the actual on board.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","8.13","Medium","","","Kongberg technician needed to attend the same // SERVICE ENGR ATTENDED AT SINGAPORE ON 22 APR. FAULT RECTIFIED.","2019-04-22","","Completed","2019-04-22","No","No","No","Internal"]
[null,null,null,null,2154,"83_2019-12-10 05:09:10.000","2019-04-12","Defect","Ship Staff","Ship Staff Insp.","Ballast Sea chest Valve cannot be opened from the Cargo Control Room. Need to open / shut using hand pump.","Deck - Machinery","Eng. / Strg. Comp.","Equipment Related","8.11","Medium","","","Technician in singapore attended // FAULT RECTIFIED.","2019-04-22","","Completed","2019-04-22","No","No","No","Internal"]
[null,null,null,null,2158,"83_2019-12-10 06:26:08.000","2019-04-12","Defect","Ship Staff","Ship Staff Insp.","NO.2 BALLAST PUMP DISCHARGE PRESSURE TRANSMITTER SHOWING PRESSURE BUT ACTUAL ITS ZERO","Elect. Mach. & Equip.","Cargo / Ballast Systems","Equipment Related","8.8","Medium","","","Pressure transmitter changed, working satisfactory.","2019-04-19","","Completed","2019-04-19","No","No","No","Internal"]
[null,null,null,null,2159,"83_2019-12-10 06:29:24.000","2019-04-12","Defect","Ship Staff","Ship Staff Insp.","Cargo seachest valve not fitted with regulator.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.11","Medium","","","REGULATOR RECEIVED & RENEWED.","2019-04-22","ATHE195090","Completed","2019-04-22","No","No","No","Internal"]
[null,null,null,null,2160,"83_2019-12-10 06:31:34.000","2019-04-12","Defect","Ship Staff","Ship Staff Insp.","1S COT Overfill alarm float stuck.\t","Elect. Mach. & Equip.","Cargo / Ballast Systems","Equipment Related","8.14","Very High","","","overhauled & Working satisfactory after overhaul. ","2019-04-16","","Completed","2019-04-16","No","No","No","Internal"]
[null,null,null,null,2161,"83_2019-12-10 06:32:58.999","2019-04-12","Defect","Ship Staff","Ship Staff Insp.","Cargo, Ballast, Pumproom valves indicators showing erratic.\t","Elect. Mach. & Equip.","Cargo / Ballast Systems","Equipment Related","8.11","Medium","","","overhauled & Working satisfactory after overhaul. ","2019-04-23","","Completed","2019-04-23","No","No","No","Internal"]
[null,null,null,null,2168,"83_2019-12-10 06:42:22.000","2019-04-12","Defect","Ship Staff","Ship Staff Insp.","7 Nos. Foam Monitor valves leaking. ","LSA / FFA","General Appearance","Equipment Related","5.38","High","","","Valves renewed.","2019-05-06","ATHE190037","Completed","2019-05-09","No","No","No","Internal"]
[null,null,null,null,2178,"83_14/10/2019 5:55:52 PM","2019-04-12","Defect","Ship Staff","Ship Staff Insp.","Port gangway collapsable rail 4 stanchions found damaged.","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.47","Medium","","","fabricated & renewed.","2019-05-18","","Completed","2019-05-20","No","No","No","Internal"]
[null,null,null,null,2183,"83_14/10/2019 6:08:27 PM","2019-04-12","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Hyd block / directional valve for mooring winch to order .","Deck - Mooring Machinery","Mooring","Equipment Related","9.14","Medium","","","Spares  ordered and repaired carry out on leaky blocks, presently no leaks.","2019-07-10","ATHE190048","Completed","2019-05-21","No","No","No","Internal"]
[null,null,null,null,2184,"83_14/10/2019 6:10:27 PM","2019-04-12","Defect","Ship Staff","Ship Staff Insp.","Ballast pp no 2 lower mech seal lekaing.\t","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.8","Medium","","","No leaks observed during loading at Juaymah.","2019-07-10","","Completed","2019-05-22","No","No","No","Internal"]
[null,null,null,null,2201,"83_14/10/2019 6:51:21 PM","2019-04-12","Defect","Ship Staff","Ship Staff Insp.","AE Purifier inoperative due to leaky sol.","E/R - Purifier","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Solenoids repalced and purifier working satisfactory.","2019-07-10","","Completed","2019-06-06","No","No","No","Internal"]
[null,null,null,null,2210,"83_15/10/2019 10:26:49 AM","2019-04-12","Defect","Ship Staff","Ship Staff Insp.","Air filter to install in the new IG  oxygen sensor line.","Inert Gas","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Filter installed.","2019-06-01","","Completed","2019-06-12","No","No","No","Internal"]
[null,null,null,null,2243,"83_15/10/2019 11:14:08 AM","2019-04-12","Defect","Ship Staff","Ship Staff Insp.","COP No.1 Electric driven system check by makers.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.18","High","","","Vacon engr to arrange with spares and for further troubleshooting- Technician joined and repaired .","2019-09-05","","Completed","2019-08-26","No","No","No","Internal"]
[null,null,null,null,2247,"83_15/10/2019 11:18:48 AM","2019-04-12","Defect","Ship Staff","Ship Staff Insp.","Rail hoses ( inlet ) side not chnaged since new building. Need to replace.\t","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Spares ordered for spare hoses.","2019-09-30","","Completed","2019-09-10","No","No","No","Internal"]
[null,null,null,null,2248,"83_15/10/2019 11:20:22 AM","2019-04-12","Defect","Ship Staff","Ship Staff Insp.","Aconis GCE module will require upgrade in due course once starts failing.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Not urgent as presently no issues faced in power management system.","2020-07-10","ATHE195031","Completed","2019-09-10","No","No","No","Internal"]
[null,null,null,null,2249,"83_15/10/2019 11:22:24 AM","2019-04-12","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Himsen DG's will require 2020 modification in due course.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Not urgent and can wait till next year.","2020-07-10","","Completed","2019-09-10","No","No","No","Internal","Owners have ordered spares in Oct and will be supplied at convene tn port."]
[null,null,null,null,2254,"83_15/10/2019 11:39:29 AM","2019-04-12","Defect","Ship Staff","Ship Staff Insp.","IG vent valve indication glass broken.","Miscellaneous","General Appearance","Equipment Related","8.25","Very High","","","Replaced with new spare received at port suez.","2019-09-15","ATHE190082","Completed","2019-10-12","No","No","No","Internal"]
[null,null,null,null,2223,"83_15/10/2019 10:45:27 AM","2019-04-13","Defect","Ship Staff","Ship Staff Insp.","Engine room vent fan No 2, impeller blade (1pc) dislodge from hub.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","RO Raised receive in Canaport, Impeller replaced and now working.","2019-07-10","ATHE190027","Completed","2019-07-29","No","No","No","Internal"]
[null,null,null,null,2193,"83_14/10/2019 6:25:32 PM","2019-04-14","Defect","Ship Staff","Ship Staff Insp.","Few strands for pumproom davit wire found broken.","Deck - Machinery","General Appearance","Equipment Related","8.5","Very High","","","Wire  renewed.","2019-06-02","","Completed","2019-06-01","No","No","No","Internal"]
[null,null,null,null,2212,"83_15/10/2019 10:29:33 AM","2019-04-15","Defect","Ship Staff","Ship Staff Insp.","B/R window wiper no.5 motor needs renewal.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","12.1","High","","","Wiper motor renewed.","2019-06-30","","Completed","2019-06-14","No","No","No","Internal"]
[null,null,null,null,2194,"83_14/10/2019 6:26:50 PM","2019-04-21","Defect","Ship Staff","Ship Staff Insp.","Yellow & Blue line AUS pneumatic discharge valve showing partially open in CCR, But actual in local the valve is fully closed.","Deck - Pipe / Fittings","General Appearance","Equipment Related","8.11","Medium","","","purged & adjusted, working well.","2019-06-03","","Completed","2019-06-05","No","No","No","Internal"]
[null,null,null,null,8435,"83_Tue Dec 10 2019 06:40:59 GMT+0000 (Coordinated Universal Time)","2019-04-21","Defect","Ship Staff","Ship Staff Insp.","Stbd Windlass Brake Cylinder leaking.","Deck - Mooring Machinery","Mooring","Equipment Related","9.2","Very High","","","Seals renewed.Brake cyl.tested and observed no leaks .","2019-05-05","","Completed","2019-05-07","No","No","No","Internal"]
[null,null,null,null,2163,"83_2019-10-12 06:33:47.000","2019-04-22","Defect","Ship Staff","Ship Staff Insp.","Oil traces found in the observation tank.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Main engine fuel oil heater no.2 found 1no tube leaking,same plugged.Again pr.tested and observed no leaks.We will keep monitoring.","2019-05-30","","Completed","2019-05-02","No","No","No","Internal"]
[null,null,null,null,2206,"83_14/10/2019 7:03:33 PM","2019-04-22","Defect","Ship Staff","Ship Staff Insp.","Boiler fuel oil pump no 2 not building sufficient pressure .","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Pump replaced with a new one .","2019-06-30","","Completed","2019-06-10","No","No","No","Internal"]
[null,null,null,null,8409,"83_Sun Nov 10 2019 15:15:09 GMT+0000 (Coordinated Universal Time)","2019-04-22","Defect","Ship Staff","Ship Staff Insp.","Emergency fire pump not building pressure.","Critical Equip.","Eng. / Strg. Comp.","Equipment Related","5.41","Very High","","","Priming pump engaging lever found broken, same welded. Pump tried out and found to be woeking satisfactory.","2019-04-23","","Completed","2019-04-23","No","No","No","Internal"]
[null,null,null,null,8410,"83_Fri Oct 11 2019 15:27:32 GMT+0000 (Coordinated Universal Time)","2019-04-22","Defect","Ship Staff","Ship Staff Insp.","OWS 3-way valve malfunctioning on test mode.","Critical Equip.","Eng. / Strg. Comp.","Equipment Related","6.17","Very High","","","Complete unit replaced by the shore w/shop UNI Marine services Singapore ( Cell + Calib.unit). Tried out and found to be working.","2019-04-23","","Completed","2019-04-23","No","No","No","Internal"]
[null,null,null,null,2173,"83_2019-12-10 06:53:02.000","2019-04-23","Defect","Ship Staff","Ship Staff Insp.","No.2 Ballast pump suction guage found inoperational.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.8","Medium","","","Suction gauge repaired  & Working satisfactory after overhaul. ","2019-05-14","","Completed","2019-05-15","No","No","No","Internal"]
[null,null,null,null,8411,"83_Sun Nov 10 2019 15:38:20 GMT+0000 (Coordinated Universal Time)","2019-04-24","Defect","Ship Staff","Ship Staff Insp.","Bilge pump not taking suc.properly.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","6.14","High","","","Assy.dismantled. Valve and valve seat having piting marks , same build up by steel putty and lapped. Pump tried out-working ok.","2019-04-24","","Completed","2019-04-24","No","No","No","Internal"]
[null,null,null,null,2146,"83_2019-10-12 03:47:47.000","2019-04-25","Defect","Ship Staff","Ship Staff Insp.","Air.cond.compressor no.2 mech.seal leaking.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Mech.seal replaced with the spare one.","2019-04-27","","Completed","2019-04-25","No","No","No","Internal"]
[null,null,null,null,2192,"83_14/10/2019 6:24:06 PM","2019-04-25","Defect","Ship Staff","Ship Staff Insp.","Pumproom davit found freezed, not swinging.","Deck - Machinery","General Appearance","Equipment Related","8.5","Very High","","","Overhauled, greased & freed.","2019-05-30","","Completed","2019-05-31","No","No","No","Internal"]
[null,null,null,null,2208,"83_15/10/2019 10:24:14 AM","2019-04-25","Defect","Ship Staff","Ship Staff Insp.","Valve remote system 3no.pressure switches faulty.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.8","Medium","","","Pressure switches replaced.","2019-06-30","","Completed","2019-06-11","No","No","No","Internal"]
[null,null,null,null,2164,"83_2019-12-10 06:35:56.999","2019-05-01","Defect","Ship Staff","Ship Staff Insp.","FWG dosing pump non functional.","E/R - Aux. Mach.","Emgcy. Systems","Equipment Related","10.32","Very High","","","Pump dismantled ,inspected and all parts cleaned.Discharge line found clogged,same cleared.","2019-05-10","","Completed","2019-05-03","No","No","No","Internal"]
[null,null,null,null,8433,"83_Tue Dec 10 2019 06:37:40 GMT+0000 (Coordinated Universal Time)","2019-05-01","Defect","Ship Staff","Ship Staff Insp.","Main engine booster pump no.2 not building sufficient pressure.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Fault traced with the relief valve.Same dismantled, o'hauled and relief v/v adjusted.","2019-05-12","","Completed","2019-05-04","No","No","No","Internal"]
[null,null,null,null,2211,"83_15/10/2019 10:28:15 AM","2019-05-05","Defect","Ship Staff","Ship Staff Insp.","Incinerator dosing pump mech. seal leaking.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Pump replaced with a new one.","2019-06-30","","Completed","2019-06-12","No","No","No","Internal"]
[null,null,null,null,2170,"83_2019-12-10 06:46:34.000","2019-05-06","Defect","Ship Staff","Ship Staff Insp.","Hydraulic leak in MW6 Winch remote opeartion pressure line .","Deck - Mooring Machinery","Mooring","Equipment Related","9.14","Medium","","","Leakage rectified.","2019-05-13","","Completed","2019-05-14","No","No","No","Internal"]
[null,null,null,null,2207,"83_15/10/2019 10:23:10 AM","2019-05-07","Defect","Ship Staff","Ship Staff Insp.","Deck seal pump no 1 mech seal leaking.","Inert Gas","Eng. / Strg. Comp.","Equipment Related","10.31","Very High","","","Pump shaft casing rings,mech.seal and shaft renewed.","2019-07-03","","Completed","2019-06-11","No","No","No","Internal"]
[null,null,null,null,8440,"83_Tue Dec 10 2019 06:50:29 GMT+0000 (Coordinated Universal Time)","2019-05-14","Defect","Ship Staff","Ship Staff Insp.","Hydraulic leak in MW2 Winch remote opeartion pressure line.","Deck - Mooring Machinery","Mooring","Equipment Related","9.14","Medium","","","Leakage rectified.","2019-05-16","","Completed","2019-05-15","No","No","No","Internal"]
[null,null,null,null,2174,"83_2019-12-10 06:54:46.000","2019-05-16","Defect","Ship Staff","Ship Staff Insp.","Composite boiler feed water pump no.2 mech.seal leaking.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Pump and motor o'hauled.Tried out-all in order.","2019-05-17","","Completed","2019-05-16","No","No","No","Internal"]
[null,null,null,null,2175,"83_2019-12-10 06:56:04.000","2019-05-16","Defect","Ship Staff","Ship Staff Insp.","DGs fuel oil heater no.2 relief valve leaking.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Relief valve dismantled,inspected and all parts cleaned.Heater put back in use and found no leaks.","2019-05-20","","Completed","2019-05-18","No","No","No","Internal"]
[null,null,null,null,2179,"83_14/10/2019 5:57:19 PM","2019-05-18","Defect","Ship Staff","Ship Staff Insp.","Fwd hyd.system no.3 pump discharge hose raptured.","Deck - Mooring Machinery","Mooring","Equipment Related","9.14","Medium","","","Hose replaced  with the spare one.","2019-07-30","","Completed","2019-05-18","No","No","No","Internal"]
[null,null,null,null,2180,"83_14/10/2019 5:59:18 PM","2019-05-19","Defect","Ship Staff","Ship Staff Insp.","HFO Purifier no.2 heater steam side gasket leaking.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Gasket renewed. No leaks in the system.","2019-05-25","","Completed","2019-05-21","No","No","No","Internal"]
[null,null,null,null,2204,"83_14/10/2019 6:55:32 PM","2019-05-20","Defect","Ship Staff","Ship Staff Insp.","NO.3 COP Separator drain line found holed.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.8","Medium","","","Fabricated & renewed.","2019-06-05","","Completed","2019-06-10","No","No","No","Internal"]
[null,null,null,null,2255,"83_15/10/2019 11:41:32 AM","2019-05-21","Defect","Ship Staff","Ship Staff Insp.","E/R signal light coloumns 2 no's in operative.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","PCBs replaced and working fine.","2019-09-30","ATHE190071","Completed","2019-09-27","No","No","No","Internal"]
[null,null,null,null,2186,"83_14/10/2019 6:13:56 PM","2019-05-23","Defect","Ship Staff","Ship Staff Insp.","Main engine L.O.Pump no.2 MCB tripping  during star/delta c/o.\t","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Fault traced with the  delta contactor,same contacts cleaned.Pump put into operation and found to be working satisfactory.","2019-05-23","","Completed","2019-05-23","No","No","No","Internal"]
[null,null,null,null,2190,"83_14/10/2019 6:20:51 PM","2019-05-23","Defect","Ship Staff","Ship Staff Insp.","13 Nos PV Valve leaking from Vaccum & pressure side.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.4","Medium","","","PV Valves overhauled.","2019-06-05","","Completed","2019-05-30","No","No","No","Internal","noted"]
[null,null,null,null,2196,"83_14/10/2019 6:43:08 PM","2019-05-23","Defect","Ship Staff","Ship Staff Insp.","3C COT IG Pressure sensor showing erratic reading.","Inert Gas","Cargo / Ballast Systems","Equipment Related","8.13","Medium","","","3C COT IG pressure sensor terminals cleaned in electronic unit - now working satisfactory. ","2019-06-05","","Completed","2019-06-04","No","No","No","Internal"]
[null,null,null,null,2187,"83_14/10/2019 6:15:42 PM","2019-05-24","Defect","Ship Staff","Ship Staff Insp.","Bunker tanks common steam return line flange gasket leaking.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Gasket renewed. ","2019-05-24","","Completed","2019-05-24","No","No","No","Internal"]
[null,null,null,null,2195,"83_14/10/2019 6:28:17 PM","2019-05-24","Defect","Ship Staff","Ship Staff Insp.","5C & 5S COT IG Pressure in Tank radar system : 5S showing pressure for 5C & Vice a versa.\t","Inert Gas","Cargo / Ballast Systems","Equipment Related","8.13","Medium","","","Wiring on 5C and 5S checked/ interchanged and now working satisfactory, It was wiring fault which was rectified. ","2019-06-05","","Completed","2019-06-04","No","No","No","Internal"]
[null,null,null,null,2101,"83_16/10/2019 6:34:09 PM","2019-06-01","Defect","Ship Staff","Ship Staff Insp.","Bunker tank overfill alarm not operational.","Miscellaneous","General Appearance","Equipment Related","10.8","Medium","","","Defective solenoid replaced with spare new received.Alarm is functional now.","2019-11-15","ATHE190089\t","Completed","2019-10-29","No","No","No","Internal"]
[null,null,null,null,2197,"83_14/10/2019 6:44:44 PM","2019-06-01","Defect","Ship Staff","Ship Staff Insp.","3P WBT Sounding pipe cap found wasted.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.8","Medium","",""," fabricated & renewed.","2019-06-08","","Completed","2019-06-06","No","No","No","Internal"]
[null,null,null,null,null,"83_5/4/2020 5:39:21 PM","2019-06-02","Defect","Ship Staff","Ship Staff Insp.","ME viscotherm erratic","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","overhauling carried out.","2020-10-10","ATHE200116","Completed","2020-10-01","No",null,null,"Internal"]
[null,null,null,null,2199,"83_14/10/2019 6:47:40 PM","2019-06-03","Defect","Ship Staff","Ship Staff Insp.","Inert gas system scrubber cooling sea water pump mech.seal leaking.","Inert Gas","Eng. / Strg. Comp.","Equipment Related","10.31","Very High","","","Mech.seal,mech.seal cover o-ring and carbon metal replaced.Pump tried out-all in order.","2019-06-08","","Completed","2019-06-05","No","No","No","Internal"]
[null,null,null,null,null,"83_5 Apr 2020 13:39:14","2019-06-05","Defect","Ship Staff","Ship Staff Insp.","SALWICO Fixed gas detection system display screen in CCR showing erratic numbers & alphabets","Miscellaneous","General Appearance","Equipment Related",8.4600000000000009,"Very High","Not Applicable","Not Applicable","Consillium technician attended the vessel and replaced the defective display with new one.","2020-07-30"," ATHE190078\t ","Completed","2020-09-16","No",null,null,"Internal"]
[null,null,null,null,2203,"83_14/10/2019 6:54:22 PM","2019-06-08","Defect","Ship Staff","Ship Staff Insp.","Stripper pump gland packing leaking.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.8","Medium","","","renewed.","2019-06-12","","Completed","2019-06-10","No","No","No","Internal"]
[null,null,null,null,2215,"83_15/10/2019 10:33:20 AM","2019-06-08","Defect","Ship Staff","Ship Staff Insp.","ME Rpm detector system 2,no.1 pick up sensor faulty.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Sensor replaced.","2019-06-20","","Completed","2019-06-17","No","No","No","Internal"]
[null,null,null,null,2216,"83_15/10/2019 10:34:31 AM","2019-06-10","Defect","Ship Staff","Ship Staff Insp.","Refer.compressor no.2 mech.seal leaking.","E/R - Aux. Mach.,Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Mech.seal renewed.","2019-06-20","","Completed","2019-06-20","No","No","No","Internal"]
[null,null,null,null,2217,"83_15/10/2019 10:35:32 AM","2019-06-11","Defect","Ship Staff","Ship Staff Insp.","5 Nos PV Valve leaking from Vaccum & pressure side.","Inert Gas","Cargo / Ballast Systems","Equipment Related","8.21","High","","","overhauled. Jon completed.","2019-06-26","","Completed","2019-06-26","No","No","No","Internal"]
[null,null,null,null,2213,"83_15/10/2019 10:30:53 AM","2019-06-14","Defect","Ship Staff","Ship Staff Insp.","Fwd Winch Hydraulic cooling line found holed.","Deck - Mooring Machinery","Mooring","Equipment Related","9.14","Medium","","","fabricated & renewed.","2019-06-20","","Completed","2019-06-15","No","No","No","Internal"]
[null,null,null,null,2105,"83_17/10/2019 6:08:53 PM","2019-06-28","Defect","Ship Staff","Ship Staff Insp.","No.1 Copt suc.pressure transmitter defective.","Cargo Mach.","Eng. / Strg. Comp.","Equipment Related","8.8","Medium","","","Spares needed to replace existing defective pressure transmitter. ","2019-09-15","ATHE190110\t","Completed","2019-11-24","No","No","No","Internal"]
[null,null,null,null,2106,"83_17/10/2019 6:10:36 PM","2019-07-01","Defect","Ship Staff","Ship Staff Insp.","All Centre cargo tanks reading in K Guage tank radar system remote display in CCR not showing correct readings & some times gets frozen.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.12","Medium","","","The hangup of the system is no more. Technician attended at Corpus Christi on 16th March.","2020-04-15"," \t ","Completed","2020-03-16","No","No","No","Internal","Minor error and Konsberg tech will be arranged at Singapore or FUJ port.  It has been attended twice in past and under monitoring."]
[null,null,null,null,2256,"83_15/10/2019 11:43:31 AM","2019-07-01","Defect","Ship Staff","Ship Staff Insp.","EVAC system pressure switch defective.\t","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Defective pressure switch replaced with new spare received at port suez.","2019-09-30","ATHE190083","Completed","2019-10-12","No","No","No","Internal"]
[null,null,null,null,10398,"83_31/1/2020 11:13:18 AM","2019-07-06","Observation","FSC Inspector","PSC Inspection","FIRE DOOR GALLEY SELF CLOSING TO BE FIXED","Accommodation ","Structural Condn. / WT integrity ","Equipment Related","10.44","Medium","Working and Living Conditions","","New door closer fitted.","2019-09-01","","Completed","2019-07-06","No","No","No","External"]
[null,null,null,null,10399,"83_31/1/2020 11:18:41 AM","2019-07-06","Observation","FSC Inspector","PSC Inspection","LATEST EDITION OF IAMSAR VOL III NOT AVAILABLE ONBOARD","Accommodation ","Structural Condn. / WT integrity ","Equipment Related","7.13","Medium","Other","","PUBLICATION RECEIVED.","2019-09-01","","Completed","2019-07-08","No","No","No","External"]
[null,null,null,null,2218,"83_15/10/2019 10:36:43 AM","2019-07-06","Defect","Ship Staff","Ship Staff Insp.","Port Anchor brake cylinder seal leaaking.","Deck - Mooring Machinery","Mooring","Equipment Related","9.2","Very High","","","Seal renewed, leak stopped. Job completed..","2019-07-15","","Completed","2019-07-12","No","No","No","Internal"]
[null,null,null,null,2219,"83_15/10/2019 10:38:07 AM","2019-07-11","Defect","Ship Staff","Ship Staff Insp.","Deck seal drain pipe flange leaking in pumproom.\t","Inert Gas","General Appearance","Equipment Related","8.25","Very High","","","New gasket replaced.","2019-07-15","","Completed","2019-07-13","No","No","No","Internal"]
[null,null,null,null,2228,"83_15/10/2019 10:52:37 AM","2019-07-12","Defect","Ship Staff","Ship Staff Insp.","X band radar scanner's motor carbon brushes worn out.","Critical Equip.","Navigation","Equipment Related","4.3","Medium","","","Carbon brushes replaced , new spares are on order.","2019-09-30","ATHE190091","Completed","2019-07-12","No","No","No","Internal"]
[null,null,null,null,2229,"83_15/10/2019 10:53:55 AM","2019-07-15","Defect","Ship Staff","Ship Staff Insp.","Hose handling crane starboard two hydraulic hoses defective.","Deck - Machinery","General Appearance","Equipment Related","8.5","Very High","","","spare hoses replaced with defective hoses.","2019-07-19","","Completed","2019-07-16","No","No","No","Internal"]
[null,null,null,null,2220,"83_15/10/2019 10:39:08 AM","2019-07-16","Defect","Ship Staff","Ship Staff Insp.","Pipe line from upper pipe duct ( s )to wilden pump for suction found holed.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.8","Medium","","","fabricated & renewed.","2019-07-19","","Completed","2019-07-18","No","No","No","Internal"]
[null,null,null,null,2107,"83_17/10/2019 6:11:57 PM","2019-07-20","Defect","Ship Staff","Ship Staff Insp.","BWTS system CLX1 defective due to water ingress while under operation .","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","6.22","Medium","","","Technician attended at USA. Initial setting carried out and system tried out.Working satisfactory.","2019-10-30"," ","Completed","2019-10-22","No","No","No","Internal"]
[null,null,null,null,2222,"83_15/10/2019 10:43:30 AM","2019-07-24","Defect","Ship Staff","Ship Staff Insp.","Port Anchor wash valve found leaking.","Deck - Pipe / Fittings","General Appearance","Equipment Related","9.2","Very High","","","Overhauled. Job completed.","2019-08-01","","Completed","2019-07-30","No","No","No","Internal"]
[null,null,null,null,2230,"83_15/10/2019 10:55:26 AM","2019-07-26","Defect","Ship Staff","Ship Staff Insp.","Rescue boat devit hydraulic motor giving 440V low insulation.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.38","Medium","","","Motor removed and re varnished and fix back, no 440V insulation alarm is activating after overhaul. ","2019-07-30","","Completed","2019-07-29","No","No","No","Internal"]
[null,null,null,null,2250,"83_15/10/2019 11:24:01 AM","2019-07-26","Defect","Ship Staff","Ship Staff Insp.","No-1 HFO Purifier vertical shaft bearing failed in service.","E/R - Purifier","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Overhaul to carry out.","2019-09-15","","Completed","2019-09-10","No","No","No","Internal","noted."]
[null,null,null,null,2221,"83_15/10/2019 10:40:15 AM","2019-07-27","Defect","Ship Staff","Ship Staff Insp.","STBD PIPE DUCT BILGE ALARM FLOAT FOUND FREEZED.","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.4","Very High","",""," OVERHAULED. Job completed.","2019-07-29","","Completed","2019-07-29","No","No","No","Internal"]
[null,null,null,null,2226,"83_15/10/2019 10:49:43 AM","2019-07-28","Defect","Ship Staff","Ship Staff Insp.","No-2 AC Compressor lube oil pump not building pressure, Discharge pressure sensor faulty.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Oil pump and pressure sensor changed with sapre, all satisfactory.","2019-07-30","","Completed","2019-07-29","No","No","No","Internal"]
[null,null,null,null,2227,"83_15/10/2019 10:50:45 AM","2019-07-30","Defect","Ship Staff","Ship Staff Insp.","Scrubber tower gas linlet pipline flange gasket blown off.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Gasket renewed, No leak present after testing. All satisfactory.","2019-07-31","","Completed","2019-07-30","No","No","No","Internal"]
[null,null,null,null,2237,"83_15/10/2019 11:06:39 AM","2019-08-03","Defect","Ship Staff","Ship Staff Insp.","ME OMD NO 9 SENSOR  FOR  FUEL PUMP GIVING FAULT ALARMS .","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.21","Medium","","","REPLACED WITH SPARE NEW ONE  Spare ordered.","2019-09-30","ATHE 190106","Completed","2019-08-20","No","No","No","Internal"]
[null,null,null,null,2232,"83_15/10/2019 10:58:03 AM","2019-08-05","Defect","Ship Staff","Ship Staff Insp.","IG to Cargo line found wasted & holed.","Inert Gas","Cargo / Ballast Systems","Equipment Related","11.4","Very High","","","Fabricated & renewed.","2019-08-15","","Completed","2019-08-08","No","No","No","Internal","Noted"]
[null,null,null,null,2234,"83_15/10/2019 11:00:22 AM","2019-08-06","Defect","Ship Staff","Ship Staff Insp.","Fabrication of One section of FWD Winch hydraulic cooling line.","Deck - Mooring Machinery","Mooring","Equipment Related","11.4","Very High","","","New line fabricated & renewed.","2019-08-15","","Completed","2019-08-14","No","No","No","Internal"]
[null,null,null,null,null,"83_5 Apr 2020 14:05:23","2019-08-06","Defect","Ship Staff","Ship Staff Insp.","Section of IG to Ballast line near Pumproom entrance found wasted & holed.\t","Inert Gas","General Appearance","Equipment Related",11.4,"Very High","Not Applicable","Not Applicable","Line was opened up, wasted section cropped and new plate welded during vessel reapirs in dry dock.","2020-09-30",null,"Completed","2020-10-23","Yes",null,null,"Internal"]
[null,null,null,null,2233,"83_15/10/2019 10:59:14 AM","2019-08-08","Defect","Ship Staff","Ship Staff Insp."," No.1 & No.2 COP AUS discharge valve pneumatic line found leaking.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.11","Medium","","","Renewed. Job completed.","2019-08-10","","Completed","2019-08-09","No","No","No","Internal"]
[null,null,null,null,null,"83_5 Apr 2020 14:07:51","2019-08-17","Defect","Ship Staff","Ship Staff Insp.","Air Ejector use for vacuum condenser found crack on end plate .","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Air ejector renewed in dry dock","2020-08-22",null,"Completed","2020-10-15","Yes",null,null,"Internal"]
[null,null,null,null,2110,"83_17/10/2019 6:17:05 PM","2019-08-20","Defect","Ship Staff","Ship Staff Insp.","Rescue boat davit hydraulic pressure dropping very fast, compensator nitrogen bladder bottle seems to be lost nitrogen gas .","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.3","Low","","","Accumulator renewed with new supplied at Kwinana. Davit tried out and found satisfactory.","2019-12-15"," ","Completed","2019-12-14","No","No","No","Internal"]
[null,null,null,null,11186,"83_5 Apr 2020 14:09:38","2019-08-20","Defect","Ship Staff","Ship Staff Insp.","New Oxygen analyzer reading of oxygen percentage is not steady causing IG deck and atmosphere valves to malfunction , Touch panel on same is defective.","Inert Gas","Eng. / Strg. Comp.","Equipment Related","8.25","Very High","","","The systems needs time provide steady reading. Asked team to have patients & observe few minutes.","2020-08-15","","Completed","2020-04-28","No","No","No","Internal"]
[null,null,null,null,2238,"83_15/10/2019 11:07:38 AM","2019-08-20","Defect","Ship Staff","Ship Staff Insp.","Fwd winch hydraulic one hydraulic hose found leaking.","Deck - Mooring Machinery","Mooring","Equipment Related","9.14","Medium","","","Same renewed.","2019-08-25","","Completed","2019-08-25","No","No","No","Internal"]
[null,null,null,null,2239,"83_15/10/2019 11:08:44 AM","2019-08-20","Defect","Ship Staff","Ship Staff Insp.","Both LT cooler sea water side are chocked with marine growth, causing LT frersh water temperature to rise.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Both LT cooler sea water side need manual cleaning of plates. Both L.T coolers chemically cleaned all parameters maintaining satisfactory .","2019-09-15","","Completed","2019-08-21","No","No","No","Internal"]
[null,null,null,null,2246,"83_15/10/2019 11:17:37 AM","2019-08-20","Defect","Ship Staff","Ship Staff Insp.","WECS computer in ECR use for motitoring/ controlling main engine parameters is shutting off (hard drive shutting off) every 15 minutes. ","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Need to replace existing WECS computer CPU with new CPU. - CPU landed at Durban and will receive back , at present original Lap top is in use.","2019-09-15","","Completed","2019-08-26","No","No","No","Internal"]
[null,null,null,null,2112,"83_17/10/2019 6:20:33 PM","2019-08-24","Defect","Ship Staff","Ship Staff Insp.","In No.2C Upper stool space located between 2C COT & 3C COT, Minor leak observed on F&A Bulkhead of 2C COT Aft entrance hatch enclosure, just forward of Frame 88 and below 2nd Transverse Bulkhead stiffner support from top.","Hull & Tanks","Structural Condn. / WT integrity ","Equipment Related","8.8","Medium","","","Temporary repairs carried out ON 27/08/19.","2019-12-31"," ","Completed","2019-11-21","No","No","No","Internal"]
[null,null,null,null,2113,"83_17/10/2019 6:21:50 PM","2019-08-24","Defect","Ship Staff","Ship Staff Insp.","\tIn No.2Stbd. Upper stool space located between 2C COT & 3C COT, Minor leak observed on F&A Bulkhead of 3C COT Fwd entrance hatch enclosure, just forward of Frame 88 and below 3rd   Transverse Bulkhead stiffner support from top. ","Hull & Tanks","Structural Condn. / WT integrity ","Equipment Related","8.8","Medium","","","Temporary repairs carried out ON 27/08/19.","2019-12-31"," ","Completed","2019-11-22","No","No","No","Internal"]
[null,null,null,null,2114,"83_17/10/2019 6:23:07 PM","2019-08-27","Defect","Ship Staff","Ship Staff Insp.","In No.4C Upper stool space located between 4C COT & 5C COT, 3 Minor leak observed on F&A Bulkhead of 4C COT Aft entrance hatch enclosure, just forward of Frame 70 and below 1ST,2nd & 3RD Transverse Bulkhead stiffner support from top.","Hull & Tanks","Structural Condn. / WT integrity ","Equipment Related","8.8","Medium","","","Temporary repairs carried out on 02/09/19.","2019-12-31"," ","Completed","2019-11-24","No","No","No","Internal"]
[null,null,null,null,2253,"83_15/10/2019 11:37:08 AM","2019-08-27","Defect","Ship Staff","Ship Staff Insp.","No:2 DG tacho fail alarm activating during operation.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Faulty speed pick up sensor changed with new spare received at port suez. working satisfactory.","2019-10-15","","Completed","2019-10-02","No","No","No","Internal"]
[null,null,null,null,2115,"83_17/10/2019 6:24:33 PM","2019-08-31","Defect","Ship Staff","Ship Staff Insp.","Main Engine auto back wash filter casing change over mechanism not working (both auto and manual side fuel pressure remains at any chosen change over leaver position) making filter cleaning impossible. Need to stop fuel system on main engine to clean filter.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","C/O mechanism opened up, alignment done & a locking plate arrangement made at the bottom of the C/O shaft to restrict its downward movement which was the cause of the rigid shaft.","2019-11-30"," ","Completed","2020-01-06","No","No","No","Internal"]
[null,null,null,null,2117,"83_17/10/2019 6:27:38 PM","2019-09-06","Defect","Ship Staff","Ship Staff Insp.","Mastriser valve ( 650 A ) opearting wheel turning freely, Suspect seat ring damage or locking pin of disc damaged .","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.25","Very High","","","Mast Riser Valve removed from place and found Seat Ring damaged. IG 41 V/V (IG to Ballast line) removed and fitted in place of Mast Riser valve. Awaiting spare seat ring for leaking IG Mast Riser Valve.","2019-11-10"," ","Completed","2019-10-07","No","No","No","Internal","Noted."]
[null,null,null,null,2252,"83_15/10/2019 11:31:31 AM","2019-09-06","Defect","Ship Staff","Ship Staff Insp.","Hydraulic leak found on Port side windlass control lever block .","Deck - Mooring Machinery","Mooring","Equipment Related","9.14","Medium","","","Rectified.","2019-10-10","","Completed","2019-09-07","No","No","No","Internal"]
[null,null,null,null,2116,"83_17/10/2019 6:26:14 PM","2019-09-07","Defect","Ship Staff","Ship Staff Insp.","STBD anchor wash pipe leaking, found pin hole.","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.4","Very High","","","Need to fabricate & Renew.","2019-11-10"," ","Completed","2019-11-10","No","No","No","Internal","Noted"]
[null,null,null,null,10118,"83_21/1/2020 10:06:18 PM","2019-09-08","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Fuel pumps High pressure pipes (from fuel pump till common rail) to tighten at various supports. They have tendency to crack in vibration","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.7","Medium","","","Done","2019-09-22","","Completed","2019-09-15","No","No","No","Internal","Checks to be carried out on monthly basis."]
[null,null,null,null,10126,"83_21/1/2020 10:33:41 PM","2019-09-08","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","All pipe supports for HP pipe for Exhaust valve to tighten. Unit 2 found loose.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Done","2019-09-23","","Completed","2019-09-15","No","No","No","Internal","Ensure this is checked during routine inspections."]
[null,null,null,null,8445,"83_15/12/2019 2:35:21 AM","2019-09-12","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Steering gear room hydraulic oil drums was arranged with direct contact with the floor plate. ","Miscellaneous","Eng. / Strg. Comp.","Inappropriate Procedure","10.29","Medium","","","Steering gear room hydraulic oil drums was arranged with a wooden pallets at the base.","2019-09-30","","Completed","2019-11-04","No","No","No","Internal"]
[null,null,null,null,10111,"83_21/1/2020 10:21:30 PM","2019-09-16","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Running hour counter to install for EVAC pumps and record every day.","Cargo Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","RUNNING HOUR COUNTER INSTALLED INSIDE PANEL","2019-10-16","","Completed","2020-02-08","No","No","No","Internal","Running hr meter will be supplied in due course."]
[null,null,null,null,10112,"83_21/1/2020 10:27:45 PM","2019-09-16","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Welding curtain is damaged in workshop and need to replace ","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","5.25","Medium","","","Requisition raised ATHE190160 in 2019. A new defect added in the same topic (ro ATHE200034). Hence closing this.","2020-08-15","","Completed","2020-05-06","No","No","No","Internal","Noted"]
[null,null,null,null,10113,"83_21/1/2020 10:43:52 PM","2019-09-16","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Salinity and Oil probe on cascade tank is not working, same to order","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","SENSOR RECIEVED AND FITTED BACK SYSTEM WORKING SATISFACTORY","2019-11-15","","Completed","2020-03-22","No","No","No","Internal","Enter new RO number for 2020. Order being followed"]
[null,null,null,null,10114,"83_22/1/2020 12:15:20 AM","2019-09-16","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","remote control lines for winch operation to be blanked & disconnected. square & round blank to order","Deck - Mooring Machinery","Mooring","Equipment Related","9.17","High","","","The leaky remote controll 2pc small lines (near 5 across) have been blanked after preparing in the E/Room workshop.","2020-03-31","","Completed","2020-02-22","No","No","No","Internal","hyd Line blanked"]
[null,null,null,null,10115,"83_21/1/2020 8:27:39 PM","2019-09-16","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Pump room start switch in CCR became faulty. Same to order and renew.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","11.1","High","","","renewed ","2019-10-15","","Completed","2019-10-14","No","No","No","Internal","Noted"]
[null,null,null,null,10116,"83_21/1/2020 8:30:13 PM","2019-09-16","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Soft patch on pipe catering overboard line just before overboard valve.  Pipe to remove and renew at earliest in ballast passage.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.31","Very High","","","Pipe repaired","2019-09-30","","Completed","2019-09-28","No","No","No","Internal","Noted"]
[null,null,null,null,10117,"83_21/1/2020 10:02:08 PM","2019-09-16","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Fuel pump LO return line / drain line to check as per RT circular 180 and report in PAL.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.7","Medium","","","Done","2019-10-15","","Completed","2019-12-12","No","No","No","Internal","Noted"]
[null,null,null,null,10119,"83_21/1/2020 10:09:32 PM","2019-09-16","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Fuel pump area to clean and paint and rectify minor lo leak","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Done","2019-09-30","","Completed","2019-09-25","No","No","No","Internal","House keeping to be prioritized at all times."]
[null,null,null,null,10120,"83_21/1/2020 10:12:23 PM","2019-09-16","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ME foundation bolt tightness to check by hyd jacks","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Done","2019-09-30","","Completed","2020-01-09","No","No","No","Internal","noted"]
[null,null,null,null,10121,"83_21/1/2020 10:15:44 PM","2019-09-16","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Steam valve for COPT governor to open and inspect for freeness. Sister vsl had trouble as valve got seized.","Cargo Mach.","Eng. / Strg. Comp.","Equipment Related","8.15","High","","","Done","2019-09-30","","Completed","2019-12-03","No","No","No","Internal"]
[null,null,null,null,10122,"83_21/1/2020 8:32:44 PM","2019-09-16","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Stern thruster electric cables to disconnect and remove.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.37","Medium","","","Done","2019-10-15","","Completed","2019-10-10","No","No","No","Internal","Noted"]
[null,null,null,null,10123,"83_21/1/2020 10:18:34 PM","2019-09-16","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Sewage treatment plant maintenance, testing, sampling log to maintain near plant.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Done","2019-09-23","","Completed","2019-09-25","No","No","No","Internal","noted."]
[null,null,null,null,10124,"83_21/1/2020 10:24:16 PM","2019-09-16","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Terminal box for both Water ballast pp to check for tightness.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.37","Medium","","","Done","2019-09-23","","Completed","2019-09-30","No","No","No","Internal","Noted"]
[null,null,null,null,10125,"83_21/1/2020 10:30:49 PM","2019-09-16","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Starting air valve solenoid to blow through at regular interval (3 months) as per RT circular","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.34","High","","","Done","2019-10-15","","Completed","2019-12-21","No","No","No","Internal","Ensure that all engineers are well aware of the procedure."]
[null,null,null,null,10127,"83_21/1/2020 10:36:59 PM","2019-09-16","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Hyd drums in steering gear room in direct metal contact with floor. To place wood or packing.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Done","2019-09-30","","Completed","2019-11-04","No","No","No","Internal","Noted."]
[null,null,null,null,10128,"83_21/1/2020 10:46:23 PM","2019-09-16","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","2 HFO bunker tanks (No 1 Stbd and No 2 Port ) to clean in upcoming voyage as per SIP . ","Hull & Tanks","Eng. / Strg. Comp.","Equipment Related","10.8","Medium","","","Done","2019-10-15","","Completed","2019-10-11","No","No","No","Internal","Noted"]
[null,null,null,null,10129,"83_21/1/2020 10:48:48 PM","2019-09-16","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","To take inventory of all manuals and highlight if any missing. ","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.12","Very High","","","Done","2019-09-30","","Completed","2019-12-15","No","No","No","Internal","Noted."]
[null,null,null,null,10130,"83_21/1/2020 10:51:59 PM","2019-09-16","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Boiler pilot burner spares to order as frequently failing due to poor insulation condition.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Spares received & renewed, now pilot burner is working in good order","2019-09-30","","Completed","2020-01-08","No","No","No","Internal","Ensure minimum spare is maintained at all times."]
[null,null,null,null,10131,"83_21/1/2020 10:56:15 PM","2019-09-16","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","COP no 3 Lub oil low pressure alarm activated at 600 rpm at 0.8 bar. The pressure switch setting to be corrected to 0.6 bar.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","8.15","High","","","Done","2019-09-30","","Completed","2019-09-19","No","No","No","Internal"]
[null,null,null,null,10132,"83_21/1/2020 11:02:28 PM","2019-09-16","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Spare HFO purifier frame to secure well on foundation in Engine room","E/R - Purifier","Eng. / Strg. Comp.","Equipment Related","6.2","High","","","Purifier secured in E/R 2nd deck","2019-10-15","","Completed","2019-09-30","No","No","No","Internal","Noted"]
[null,null,null,null,10133,"83_21/1/2020 10:40:16 PM","2019-09-16","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Boiler emergency firing procedure to make and all engineers to train / familiarize.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","8.37","High","","","Done","2019-09-23","","Completed","2019-09-23","No","No","No","Internal","Ensure same is posted near the Boiler for easy reference."]
[null,null,null,null,10134,"83_21/1/2020 10:59:26 PM","2019-09-16","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Many drain scuppers in engine room are choke. To clear them, if require cut and put flanges","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","6.2","High","","","Done","2019-12-15","","Completed","2019-12-20","No","No","No","Internal","Noted"]
[null,null,null,null,10135,"83_21/1/2020 11:14:10 PM","2019-09-16","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Singapore bunkering procedure guideline not onboard. To supply","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","4.1","High","","","Bunkering procedure received.","2019-11-15","","Completed","2019-12-08","No","No","No","Internal","Noted"]
[null,null,null,null,10137,"83_21/1/2020 11:17:35 PM","2019-09-16","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","PMS to incorporate spare parts from office side by Valad","Documentation","Eng. / Strg. Comp.","Equipment Related","10.12","Very High","","","Done","2019-11-15","","Completed","2019-12-05","No","No","No","Internal","followed with valad and now spares populated."]
[null,null,null,null,10138,"83_21/1/2020 11:33:39 PM","2019-09-16","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","fwd & aft hyd power pack hyd hoses are leaking & requires immediate replacement.","Deck - Mooring Machinery","Mooring","Equipment Related","9.14","Medium","","","hoses replaced with newly received hoses.","2019-09-30","","Completed","2019-10-04","No","No","No","Internal","Actions noted."]
[null,null,null,null,10139,"83_21/1/2020 11:37:01 PM","2019-09-16","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","windlass gear teeth were found dry. same to be greased.","Critical Equip.","Structural Condn. / WT integrity ","Equipment Related","9.2","Very High","","","windlass gear teeth greased.","2019-10-03","","Completed","2019-10-03","No","No","No","Internal","This action has to be done as per PMS and followed up."]
[null,null,null,null,10140,"83_21/1/2020 11:41:32 PM","2019-09-16","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","the stbd crane hydraulic hoses end connectors getting rusty. same to be brushed & apply denso tape.","Deck - Machinery","Structural Condn. / WT integrity ","Equipment Related","8.5","Very High","","","denso tape applied at the connectors.","2019-09-18","","Completed","2019-09-18","No","No","No","Internal","During monthly inspections ensure same is checked and action to be taken immediately."]
[null,null,null,null,10141,"83_21/1/2020 11:11:15 PM","2019-09-16","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Bilge pump valve seats are repaired by devcon and performance is poor. Spares on order and need urgently","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","6.14","High","","","Done","2019-10-15","","Completed","2019-11-01","No","No","No","Internal","Noted."]
[null,null,null,null,10142,"83_21/1/2020 11:45:31 PM","2019-09-16","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","stay wires to be greased & apply with denso tape.","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","Equipment Related","11.5","Medium","","","greased & denso tape applied.","2019-09-17","","Completed","2019-09-17","No","No","No","Internal"]
[null,null,null,null,10143,"83_21/1/2020 11:49:24 PM","2019-09-16","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","mast riser vent valve reported leak. same to be repaired or supply new at next port.","Inert Gas","Cargo / Ballast Systems","Equipment Related","8.25","Very High","","","defective valve replaced.","2019-09-30","","Completed","2019-10-01","No","No","No","Internal","To prevent re-occurrence kindly check the same during monthly inspections."]
[null,null,null,null,10144,"83_21/1/2020 11:53:23 PM","2019-09-16","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","the electric conduct line pipes are pending to be painted red brown. to complete same after surafce preparation. to supply spray painter for good quality.","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.5","Medium","","","conduvt line painting complted.","2019-12-15","","Completed","2019-11-09","No","No","No","Internal","Noted"]
[null,null,null,null,10145,"83_21/1/2020 11:57:03 PM","2019-09-16","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","educators to try out for various void spaces.","Deck - Machinery","Cargo / Ballast Systems","Equipment Related","8.8","Medium","","","void spaces educator tried out.","2019-10-01","","Completed","2019-11-01","No","No","No","Internal","Ensure this is carried out as per PMS schedule."]
[null,null,null,null,10146,"83_22/1/2020 12:00:31 AM","2019-09-16","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","rust spots / stains on both manifold area & its pipes to be attended.","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","Equipment Related","11.4","Very High","","","derusting & painting of manifold area pipes carried out.","2019-10-15","","Completed","2019-10-16","No","No","No","Internal","To prevent re-occurrence kindly check the same during monthly inspections."]
[null,null,null,null,10147,"83_22/1/2020 12:06:57 AM","2019-09-16","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","life boat davit RAM pin grease points dry, same to grease.","LSA / FFA","Emgcy. Systems","Equipment Related","5.29","High","","","greasing carried out.","2019-09-30","","Completed","2019-10-19","No","No","No","Internal","Vessel greasing schedule to be followed at all times."]
[null,null,null,null,10148,"83_22/1/2020 12:11:06 AM","2019-09-16","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","the rope retaining the life boat grab wires should be secured properly so that it can be released quickly after launching.","LSA / FFA","Emgcy. Systems","Equipment Related","5.29","High","","","job completed.","2019-09-30","","Completed","2019-10-18","No","No","No","Internal","Checks to be carried out during routine inspections."]
[null,null,null,null,10149,"83_22/1/2020 12:18:45 AM","2019-09-16","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","gangway air lubricator for stbd side to renew with onboard spare.","Deck - Machinery","Structural Condn. / WT integrity ","Equipment Related","5.47","Medium","","","air lubricator renewed.","2019-09-30","","Completed","2019-10-03","No","No","No","Internal","To prevent re-occurrence kindly check the same during monthly inspections."]
[null,null,null,null,10150,"83_22/1/2020 12:21:32 AM","2019-09-16","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp."," M4 winch control block is cut & repaired. same to order & replace.M","Deck - Mooring Machinery","Mooring","Equipment Related","9.17","High","","","control block replaced.","2019-12-15","","Completed","2019-12-10","No","No","No","Internal","Noted"]
[null,null,null,null,10151,"83_22/1/2020 12:27:37 AM","2019-09-16","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Crew requested entertainment items, same to be supplied at convient port.","Miscellaneous","Crew Management","Behaviour Based","11.8","Low","","","supplied.","2019-09-30","","Completed","2019-09-24","No","No","No","Internal"]
[null,null,null,null,10152,"83_22/1/2020 12:30:58 AM","2019-09-16","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ventilator fan to derust & paint.","Deck - Machinery","Structural Condn. / WT integrity ","Equipment Related","11.7","High","","","derusted & painted.","2019-09-30","","Completed","2019-10-14","No","No","No","Internal","Noted"]
[null,null,null,null,10153,"83_22/1/2020 12:03:18 AM","2019-09-16","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","few mooring wires found lacking grease.","Deck - Mooring Machinery","Mooring","Equipment Related","9.17","High","","","mooring wires greased.","2019-10-15","","Completed","2019-10-09","No","No","No","Internal","PMS schedule to be followed at all times"]
[null,null,null,null,10154,"83_22/1/2020 12:36:06 AM","2019-09-16","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","life raft embarkation ladder canvas cover is torn & performance is poor.","LSA / FFA","Safety / LSA / FFA","Inappropriate Procedure","5.14","Very High","","","completd","2019-09-30","","Completed","2019-10-02","No","No","No","Internal","Noted"]
[null,null,null,null,2251,"83_15/10/2019 11:25:11 AM","2019-09-16","Defect","Ship Staff","Ship Staff Insp.","Control air rubber hose for COP No.2 found leaked during \n\nroutine inspection after departure discharge Sikka, India.\n\n\t","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.8","Medium","","","Need to Replace the rubber pipe.","2019-09-30","","Completed","2019-09-18","No","No","No","Internal"]
[null,null,null,null,11214,"83_05-Apr-20 02:18:18","2019-09-16","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","NEW CLOCK FITTED AT BRIDGE WITH DIMMER AND WORKING FINE.","Cargo Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","RUNNING HOUR COUNTER INSTALLED INSIDE PANEL","2019-09-16","","Completed","2020-02-08","No","No","No","Internal"]
[null,null,null,null,2261,"83_17/10/2019 6:41:50 PM","2019-09-22","Defect","Ship Staff","Ship Staff Insp.","Both No-1 and No-2 air condition compressor to repair after Both failed in service.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Vessel received two new aircondition compressor at Suez and both compressor changed to new one. ","2019-10-15","","Completed","2019-10-14","No","No","No","Internal","Pls highlight duty engr to take proper rounds and monitor the parameters."]
[null,null,null,null,2260,"83_17/10/2019 6:40:36 PM","2019-10-01","Defect","Ship Staff","Ship Staff Insp.","Galley overboard line developed a pin hole just next to overboard valve, section of pipe need to be replaced.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.31","Very High","","","Galley overboard pipe section renewed.","2019-10-02","","Completed","2019-10-02","No","No","No","Internal"]
[null,null,null,null,2257,"83_15/10/2019 11:45:58 AM","2019-10-07","Defect","Ship Staff","Ship Staff Insp.","Vapour return line STBD side aft main valve actuator found cracked on prior arrival load port checks.","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.4","Very High","","","Actuator replaced with spare actuator available on board.","2019-10-08","","Completed","2019-10-07","No","No","No","Internal"]
[null,null,null,null,2121,"83_17/10/2019 6:33:26 PM","2019-10-11","Defect","Ship Staff","Ship Staff Insp.","Air con comressor no-1 suction gas temperature sensor defective\t.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Spare received, same replaced. Working satisfactory.","2020-04-15"," Requisition ATHE190152 ","Completed","2020-01-16","No","No","No","Internal"]
[null,null,null,null,null,"83_5 Apr 2020 14:19:30","2019-10-11","Defect","Ship Staff","Ship Staff Insp.","Main air compressor no-1 and 2 shows signs of crankcase contamination with water, Oil need changing freqently.","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Compressor overhauling done,No abnormalities observed.","2020-08-15",null,"Completed","2020-08-11","No",null,null,"Internal"]
[null,null,null,null,8450,"83_Mon Mar 11 2019 01:25:37 GMT+0000 (Coordinated Universal Time)","2019-10-26","Defect","Ship Staff","Ship Staff Insp.","Foam Station Telephone - found not working /operational","Elect. Mach. & Equip.","Communication","Equipment Related","10.32","Very High","","","Faulty mic replaced with spare one. tried out working fine.","2019-11-15","","Completed","2019-12-01","No","No","No","Internal"]
[null,null,null,null,8449,"83_15/12/2019 3:00:53 AM","2019-10-28","Defect","Ship Staff","Ship Staff Insp.","Main Engine F.O Booster pump No 2 - Found making abnormal noise. Pump to be opened up and checked. ","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Re-Conditioned pump complete (with motor) was receieved at Kwinana port. Same was installed and pump tried out.Found satisfactory.","2019-12-15","","Completed","2019-12-14","No","No","No","Internal","Noted. Need to be more careful with pump operation."]
[null,null,null,null,8446,"83_Mon Mar 11 2019 01:33:01 GMT+0000 (Coordinated Universal Time)","2019-10-29","Defect","Ship Staff","Ship Staff Insp.","Aux.Boiler No: 1 - Found Top Manhole gasket leaking when boiler is pressurized","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Boiler to be de-pressurized and Manhole gasket renewed.","2019-11-15","","Completed","2019-11-06","No","No","No","Internal"]
[null,null,null,null,null,"83_Sun Nov 03 2019 01:37:34 GMT+0000 (Coordinated Universal Time)","2019-10-30","Defect","Ship Staff","Ship Staff Insp.","Aux Boiler No 1 and 2 - Gauge glass illumination lights faulty (3 nos)","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Renewed with new spare","2020-09-30","ATHE190197","Completed","2020-10-20","No",null,null,"Internal"]
[null,null,null,null,9734,"83_17/1/2020 5:16:59 PM","2019-11-03","Defect","Ship Staff","Ship Staff Insp.","GMDSS POWER MODULE 240 FOR inmarsat C not working","Navigation - GMDSS & Communication","Communication","Equipment Related","4.24","High","","","Spare received, same renewed. Working satisfactory.","2019-12-31","Requisition raised ATHE195147","Completed","2019-12-23","No","No","No","Internal"]
[null,null,null,null,8447,"83_15/12/2019 2:43:00 AM","2019-11-05","Defect","Ship Staff","Ship Staff Insp.","No : 1 AC Compressor Pin hole on compressor HP discharge valve line.Hot work to be carried out.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","No : 1 AC Compressor isolated , gas collected in recovery bottled and  Pin hole on compressor HP discharge valve line brazed. Hot work permission obtained from office for the same and Hot work permit  made.","2019-11-30","","Completed","2019-11-15","No","No","No","Internal"]
[null,null,null,null,8453,"83_15/12/2019 3:42:21 AM","2019-11-14","Defect","Ship Staff","Ship Staff Insp.","Elevato door controller PCB found defective. Door was found not opening and close limit switch LED was seen continuously  ON even when door was open. ","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Replaced PCB with spare received at Kwinana. PCB calibrated and elevator tried out. Found satisfactory. ","2019-12-15","","Completed","2019-12-12","No","No","No","Internal"]
[null,null,null,null,null,"83_5 Apr 2020 14:36:05","2019-11-20","Non Conformity","Ship Staff","Ship Staff Insp.","No Brake testing kit available for mooring winches","Deck - Machinery","Mooring","Equipment Related",9.6999999999999993,"Medium","Not Applicable","Not Applicable","New BHC test kit was supplied in dry dock.","2020-06-15","ATHE200045","Completed","2020-10-20","No",null,null,"Internal"]
[null,null,null,null,8448,"83_15/12/2019 2:50:31 AM","2019-11-30","Defect","Ship Staff","Ship Staff Insp.","Main Steam stop valve (line valve) of  #1 and #2 boilers - Bonnet gasket leaking","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Main Steam stop valve (line valve) of  #1 and #2 boilers - Bonnet gaskets renewed. Boilers depressurized valve bonnet opened and gasket renewed.","2019-12-06","","Completed","2019-12-04","No","No","No","Internal"]
[null,null,null,null,8451,"83_15/12/2019 3:32:35 AM","2019-12-01","Defect","Ship Staff","Ship Staff Insp.","Main Engine - Fuel Pump #2 Actuator is found sluggish. To be opened up and carbon brushes renewed. ","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Actuator carbon brushes received at Kwinana port.Same was used and Fuel pump # 2 Actuator overhauled. Engine tried out and found satisfactory.","2019-12-15","","Completed","2019-12-12","No","No","No","Internal"]
[null,null,null,null,9732,"83_17/1/2020 4:55:47 PM","2019-12-05","Defect","Ship Staff","Ship Staff Insp.","ME servo oil pupmp compensator solenoid valve faulty","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Spare received, same renewed. working satisfactory","2020-01-01","Requisition raised ATHE195147","Completed","2019-12-14","No","No","No","Internal"]
[null,null,null,null,8788,"83_21/12/2019 8:41:29 AM","2019-12-10","Defect","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","Rescue boat launching deck stanchions are are secured with tiger rope. KOCH SIRE inspector advised should have wire rope securing.","LSA / FFA","Safety / LSA / FFA","Inappropriate Procedure","5.11","Low","",""," will be done at convient.","2019-12-31","","Completed","2019-12-13","No","No","No","External"]
[null,null,null,null,8789,"83_21/12/2019 8:45:18 AM","2019-12-10","Defect","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","Officer's smoking room exhaust stencil found faded.","Miscellaneous","General Appearance","Inappropriate Procedure","5.1","Very High","","","TO re stencil the space.","2019-12-31","","Completed","2019-12-27","No","No","No","External"]
[null,null,null,null,8791,"83_Fri Dec 20 2019 18:37:11 GMT+0000 (Coordinated Universal Time)","2019-12-10","Defect","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","Rescue boat davit operation on stored hydraulic power was very slow & sluggish.","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.29","High","","","Shore technician from denray Marine attendenance onboard on 14 Dec 2019 at Outer Anchorage, Fremantle, Western Australia after completion of first STS. Rescue boat davit found to be working good after shore servicing.","2020-01-10","","Completed","2019-12-14","No","No","No","External","noted."]
[null,null,null,null,8792,"83_Fri Dec 20 2019 18:41:44 GMT+0000 (Coordinated Universal Time)","2019-12-10","Defect","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","Emergency light for rescue boat & one emergency light for the free fall life boat were not working. same was repaired before the end of inspection.","Elect. Mach. & Equip.","Emgcy. Systems","Equipment Related","5.18","High","","","Rectified before completion of inspection.","2019-12-11","","Completed","2019-12-10","No","No","No","External"]
[null,null,null,null,null,"83_3/2/2020 1:19:19 PM","2019-12-10","Defect","Ship Staff","Ship Staff Insp.","ME SERVO RAIL HOLDING DOWN BOLTS CRACKED, ALSO RAIL UNIT SUPPORTING WEBS CRACKED.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","job completed in dry dock","2020-10-10",null,"Completed","2020-10-25","No",null,null,"Internal"]
[null,null,null,null,8452,"83_15/12/2019 3:37:07 AM","2019-12-13","Defect","Ship Staff","Ship Staff Insp.","Main Engine L.O pump # 2 - MCCB was found tripping while starting. Problem to be investigated.\t","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Found timer for Y-D change over timer faulty. Same renewed with spare one. pump tried out found working satisfactory.","2019-12-14","","Completed","2019-12-14","No","No","No","Internal"]
[null,null,null,null,9733,"83_17/1/2020 5:05:16 PM","2019-12-13","Defect","Ship Staff","Ship Staff Insp.","# 1 ACS 2 controller, malfuntioning","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Replace the controller with a spare one, working satisfactory.","2019-12-31","","Completed","2019-12-14","No","No","No","Internal"]
[null,null,null,null,11191,"83_5 Apr 2020 14:28:00","2019-12-15","Defect","Ship Staff","Ship Staff Insp.","Scrubber Tower - High level float alarm was found not fuctioning during routine checks. Found float missing.","Inert Gas","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Requisition ATHE190216 received and float renewed, tried out. Working satisfactory. ","2020-07-15","ATHE190216","Completed","2020-05-25","No","No","No","Internal"]
[null,null,null,null,8386,"83_15/12/2019 3:55:10 AM","2019-12-15","Defect","Ship Staff","Ship Staff Insp.","ME Local Manoeuvring platform - Telephone booth rotating strobe lights and bell found broken and not fuctional. Same to be replaced.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.37","Medium","","","Requisition ATHE190218 received, same renewed. Working satisfactory.","2020-08-15","ATHE190218","Completed","2020-06-04","No","No","No","Internal","noted and will arrange at earliest. Vessel must have raised new requisition in 2020. Mention the new number."]
[null,null,null,null,8388,"83_15/12/2019 8:22:39 PM","2019-12-15","Defect","Ship Staff","Ship Staff Insp.","The indication for the Fire isolation v/v not moving (near 2C). Though the valve is free to operate and it is closing/opeing properly.","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.38","High","","","To be overhaued the indication mechanism.","2020-02-14","","Completed","2020-01-13","No","No","No","Internal","Pls plan at earliest as FFA item."]
[null,null,null,null,8389,"83_15/12/2019 8:45:31 PM","2019-12-15","Other","Ship Staff","Ship Staff Insp.","About 75% of the mooring winchs \"Distance nut\" got larger value. (As the brakes are fully open, the bottom part of the brake band should rest/touch the distance nut, which is not happending due to incorrect setting).","Deck - Mooring Machinery","Mooring","Industry Issue","9.14","Medium","","","Distance nut to be adjusted, so that it just touch when brake is fully open.","2020-01-14","","Completed","2020-01-15","No","No","No","Internal"]
[null,null,null,null,null,"83_5 Apr 2020 14:24:33","2019-12-15","Breakdown","Ship Staff","Ship Staff Insp.","Pumpromm fix gas detection system screen in the CCR dead.","Miscellaneous","Cargo / Ballast Systems","Equipment Related",8.4600000000000009,"Very High","Not Applicable","Not Applicable","Consillium technician attaended the vessel at Singapore and replaced the defective parts, system now working satisfactorily.","2020-07-25",null,"Completed","2020-09-17","No",null,null,"Internal"]
[null,null,null,null,null,"83_Sun Dec 15 2019 10:06:29 GMT+0000 (Coordinated Universal Time)","2019-12-15","Defect","Ship Staff","Ship Staff Insp.","Cargo oil tank 2C ullage/pressure sensor & Slop-P & S temperature sensor not working.","Cargo Mach.,Inert Gas","Cargo / Ballast Systems","Equipment Related",8.25,"Very High","Not Applicable","Not Applicable","Service technician visisted in Singapore on 16 Sept 2020, issue is resolved.","2020-07-05",null,"Completed","2020-09-17","No",null,null,"Internal"]
[null,null,null,null,null,"83_05-Apr-20 01:57:04","2019-12-15","Defect","Ship Staff","Ship Staff Insp.","3 nos of caps for deck air valves missing from location (Forcastle deck-1pc, P/Room COP deck-1pc, Main dk-1)","Deck - Pipe / Fittings","General Appearance","External Factors",11.7,"High","Not Applicable","Not Applicable","Spares received and put in place.","2020-09-01","ATHE200165","Completed","2020-10-08","No",null,null,"Internal"]
[null,null,null,null,null,"83_5/4/2020 5:45:16 PM","2019-12-15","Defect","Ship Staff","Ship Staff Insp.","Various wasted pipe support angle bars on main deck","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","Equipment Related",11.1,"High","Not Applicable","Not Applicable","All wasted pipe supports renewed.","2020-09-15",null,"Completed","2020-11-05","Yes",null,null,"Internal"]
[null,null,null,null,8790,"83_25/12/2019 9:46:10 AM","2019-12-23","Defect","Ship Staff","Ship Staff Insp.","Lashing ropes for bunker valves on port manifold is missing.","Miscellaneous","Cargo / Ballast Systems","Industry Issue","8.11","Medium","","","To fix new lashing ropes for the missing one.","2019-12-31","","Completed","2019-12-29","No","No","No","Internal"]
[null,null,null,null,9735,"83_17/1/2020 5:22:42 PM","2020-01-01","Defect","Ship Staff","Ship Staff Insp.","PORT bridge wing rudder angle indicator found not working","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Broken cables renewed","2020-01-31","","Completed","2020-01-02","No","No","No","Internal"]
[null,null,null,null,9730,"83_15/1/2020 4:26:30 AM","2020-01-05","Observation","Ship Staff","Ship Staff Insp.","FORECASTLE DECK WALKWAY TO FOC'LE STORE STANCHION HOLDERS ARE PROVIDED. HOWEVER, STANCHIONS ARE NOT AVAILABLE ONBOARD.","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","Inappropriate Procedure","11.3","Medium","","","Staunchions fixed & kept forward.","2020-02-05","ATHE200042 & ATHE205012","Completed","2020-04-10","No","No","No","Internal","Mention the requisition number."]
[null,null,null,null,11215,"83_5 Apr 2020 14:31:08","2020-01-11","Breakdown","Ship Staff","Ship Staff Insp.","COP NO.2 AUS SEPARATOR  DP LEVEL TRANSMITTER OUT OF ORDER.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.8","Medium","","","Old one made working after inspection/cleaning components.","2020-02-05","","Completed","2020-02-23","No","No","No","Internal"]
[null,null,null,null,11193,"83_5 Apr 2020 14:40:01","2020-01-15","Non Conformity","Ship Staff","Ship Staff Insp.","NO BLANKS AVAILABLE FOR 12\" CARGO & VAPOUR  REDUCERS.","Deck - Pipe / Fittings","Cargo / Ballast Systems","External Factors","8.25","Very High","","","NEW BLANKS RECEIVED AT KWINANA","2020-07-05","ATHE200041","Completed","2020-05-25","No","No","No","Internal"]
[null,null,null,null,11216,"83_05-Apr-20 02:13:38","2020-01-20","Observation","Ship Staff","Ship Staff Insp.","# 1 BALLAST WATER PUMP UPPER MECHANICAL SEAL FOUND LEAKING","Deck - Machinery","Cargo / Ballast Systems","Equipment Related","8.19","High","","","MECHANICAL SEAL RENEWED","2020-05-01","","Completed","2020-02-22","No","No","No","Internal"]
[null,null,null,null,10402,"83_2/2/2020 2:07:51 PM","2020-01-22","Defect","Ship Staff","Ship Staff Insp.","IG Main Line found wasted & Leaking inside pipe duct.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.3","Very High","","","Cold work done (devcon after surface preparation). Soap test done after repair with 700mmwg IG pressure and holding good.","2020-02-02","","Completed","2020-01-24","No","No","No","Internal"]
[null,null,null,null,10401,"83_30/1/2020 1:02:34 PM","2020-01-24","Breakdown","Ship Staff","Ship Staff Insp.","Bridge AC unit not colling properly.","Elect. Mach. & Equip.","Navigation","Equipment Related","10.23","Medium","","","Found Power supply cable lug disconnected from the A/C compressor unit terminal.All the lugs renewed, found working satisfactory.","2020-02-02","","Completed","2020-01-27","No","No","No","Internal"]
[null,null,null,null,10397,"83_01-Feb-20 17:57:03","2020-01-25","Defect","Ship Staff","Ship Staff Insp.","Clock illumination is not working","Navigation - Others","Navigation","Equipment Related","11.9","Low","","","NEW CLOCK FITTED AT BRIDGE WITH DIMMER AND WORKING FINE.","2020-02-25","","Completed","2020-02-15","No","No","No","Internal","Carry out trouble shooting and revert with action plan."]
[null,null,null,null,10400,"83_3/2/2020 5:31:42 AM","2020-01-25","Defect","Ship Staff","Ship Staff Insp.","# 1 Air handling unit fan starter panel MCCB breaker damage","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","MCCB breaker, OCR & contactors renewed","2020-01-25","","Completed","2020-01-25","No","No","No","Internal"]
[null,null,null,null,12108,"83_17-Apr-20 02:39:37","2020-01-30","Defect","Ship Staff","Ship Staff Insp.","Port side bridge wing rudder angle indicator out by 2 deg. ","Navigation - Others","Navigation","Equipment Related","10.39","High","","","The existing one repaired & the differnce is Nil. The new spare did not consume & kept spare (ATHE200071).","2020-07-30","ATHE200071","Completed","2020-05-29","No","No","No","Internal"]
[null,null,null,null,null,"83_10-Apr-20 12:02:28","2020-02-04","Defect","Ship Staff","Ship Staff Insp.","NO.2 VHF HANDSET  CABLE DAMAGE ","Navigation - Others","Navigation","Equipment Related",null,null,"Not Applicable","Not Applicable","New handset was supplied in Singapore, old damaged handset replaced with new one.","2020-08-29","ATHE205018","Completed","2020-09-17","No",null,null,"Internal"]
[null,null,null,null,11217,"83_05-Apr-20 02:22:57","2020-02-05","Observation","Class Surveyor","Others (Eg. Insurance etc.)","Training for BWM convention & management plan to be carried out to all crew members.\n\n(observed that an entry made on Ballast record book on date 15/04/2019 to 14/05/2019 under code “Ballast Details”. It was recorded as “BWE (ER),” instead of “BWE (SE)”.","Hull & Tanks","Cargo / Ballast Systems","Knowledge Based","5.34","Low","","","Training to be carried out.","2020-02-25","","Completed","2020-02-15","No","No","No","External"]
[null,null,null,null,10992,"83_15/2/2020 4:00:54 PM","2020-02-05","Defect","Class Surveyor","Others (Eg. Insurance etc.)","# 1 BALLAST WATER PUMP UPPER MECHANICAL SEAL FOUND LEAKING","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.19","High","","","MECHANICAL SEAL RENEWED","2020-05-01","","Completed","2020-02-22","No","No","No","External"]
[null,null,null,null,10993,"83_15/2/2020 3:39:17 PM","2020-02-05","Observation","Class Surveyor","Others (Eg. Insurance etc.)","EMERGENCY D/G FREQUENCY FOUND TO BE 62 WHILE TEST RUNNING","Critical Equip.","Emgcy. Systems","Equipment Related","10.5","Low","","","FREQUENCY ADJUSTED TO 60.5 Hz","2020-02-15","","Completed","2020-02-08","No","No","No","External"]
[null,null,null,null,10994,"83_15/2/2020 3:47:54 PM","2020-02-05","Defect","Class Surveyor","OM Insp. (Eg. SIRE / CDI etc.)","SEWAGE PLANT OZONE DOSING PUMP FOUND TRIPPING ON OVERLOAD","Elect. Mach. & Equip.","MARPOL Related","Equipment Related","10.32","Very High","","","DOSING PUMP OPENED, LINE CLEARED OF DIRT & TRIED OUT. FOUND SATISFACTORY.","2020-02-15","","Completed","2020-02-08","No","No","No","External"]
[null,null,null,null,10995,"83_15/2/2020 3:56:31 PM","2020-02-05","Defect","Class Surveyor","Others (Eg. Insurance etc.)","INCINERATOR\n\n1. ALARM LAMP NOT WORKING\n\n2. OUTSIDE BOOTOM TO BE CLEANED & DRIP TRAY TO BE REMOVED\n\n3. FURNACE DOOR REFRACTORY TO BE REPAIRED. ","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.1","Medium","","","1. ALARM LAMP RENEWED\n\n2. INCINERATOR BOTTOM AREA CLEANED & DRIP TRAY REMOVED.\n\n3. FURNACE DOOR REFRACTORY RENEWED.","2020-02-20","","Completed","2020-02-15","No","No","No","External"]
[null,null,null,null,10996,"83_17/2/2020 12:02:04 AM","2020-02-05","Observation","Class Surveyor","Others (Eg. Insurance etc.)","Training for BWM convention & management plan to be carried out to all crew members.\n\n(observed that an entry made on Ballast record book on date 15/04/2019 to 14/05/2019 under code “Ballast Details”. It was recorded as “BWE (ER),” instead of “BWE (SE)”.","Miscellaneous","Crew Management","Knowledge Based","5.34","Low","","","Training to held.","2020-02-25","","Completed","2020-02-15","No","No","No","External"]
[null,null,null,null,null,"83_10-Apr-20 11:56:39","2020-02-05","Defect","Others (Eg. Insurance etc.)","Others (Eg. Insurance etc.)","Gyro Compass Operation Unit Display Error","Navigation - Others","Navigation","Equipment Related",null,null,"Not Applicable","Not Applicable","Troubleshooting carried out by technician, unit working satisfactorily now.","2020-07-29","ATHE205019","Completed","2020-09-17","No",null,null,"Internal"]
[null,null,null,null,11218,"83_05-Apr-20 02:04:51","2020-02-20","Non Conformity","Ship Staff","Ship Staff Insp.","There is no audible or visual alarm provided for Cargo tank remote gauging system for tank pressure ( secondary means of venting) & high level alarm. No means to test the same.","Cargo Mach.,Hull & Tanks","Cargo / Ballast Systems","Equipment Related","8.19","High","","","Technician visited at Corpus Christi & rectified. Now audible & visual alarm activates in CCR","2020-02-28","","Completed","2020-03-16","No","No","No","Internal"]
[null,null,null,null,11222,"83_6/4/2020 7:43:41 AM","2020-03-02","Observation","Owner / Marine / Tech. Suptd.","Bunkering Audit","12.04.08.014.00 Bunkering safety checklist Section # 3 Checks by barge prior berthing ticked by own vessel. ","Miscellaneous","Eng. / Strg. Comp.","Inappropriate Procedure","","","","","Persons involved in Bunkering instructed to get the checklist filled by the Bunker barge","2020-03-10","","Completed","2020-03-04","No","No","No","Internal"]
[null,null,null,null,11194,"83_5/4/2020 8:01:31 PM","2020-03-03","Defect","Ship Staff","Ship Staff Insp.","80% of Cow machines not turing when cowed in Canaport on 01-02 March 2020.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.34","High","","","Overhauling of faulty COW machine after removing from tanks. All machines gearbox lubricated. Tested and moving easily.","2020-06-25","","Completed","2020-05-06","No","No","No","Internal"]
[null,null,null,null,11219,"83_05-Apr-20 02:08:40","2020-03-03","Observation","Owner / Marine / Tech. Suptd.","ISM Audit","No entries in the CCR movement book to show entries as per (12.21.03.001.00) - \n\nDischarging operation carried out on 26 Dec 2019 with vapor balancing line connected.\n\n","Deck - Pipe / Fittings","Cargo / Ballast Systems","Human Error","","","","","All Deck officer's familiarized with checklist & breifed to make appropriate entries prior using vapor line","2020-04-03","","Completed","2020-03-27","No","No","No","Internal"]
[null,null,null,null,11220,"83_6/4/2020 7:46:14 AM","2020-03-03","Observation","Owner / Marine / Tech. Suptd.","Bunkering Audit","Time interval for repetitive checks not mentioned in 12.04.08.014.00 Bunkering safety checklist used for LSMGO bunkering on 30.10.2019. ","Miscellaneous","Eng. / Strg. Comp.","Inappropriate Procedure","","","","","Corrected","2020-03-10","","Completed","2020-03-04","No","No","No","Internal"]
[null,null,null,null,11223,"83_05-Apr-20 02:06:39","2020-03-03","Observation","Owner / Marine / Tech. Suptd.","ISM Audit","Technician visited at Corpus Christi & rectified. Now audible & visual alarm activates in CCR","Deck - Pipe / Fittings","Cargo / Ballast Systems","Human Error","","","","","Completion time entered & all officers breifed.","2020-04-03","","Completed","2020-03-05","No","No","No","Internal"]
[null,null,null,null,11221,"83_05-Apr-20 02:02:18","2020-03-20","Observation","Ship Staff","Ship Staff Insp.","Calibration gas onboard exausted & no more available for calibrating gas instruments.","Miscellaneous","Safety / LSA / FFA","External Factors","5.23","Very High","","","Calibration gas received & instruments calibrated","2020-03-25","ATHE200088","Completed","2020-03-20","No","No","No","Internal"]
[null,null,null,null,11195,"83_5/4/2020 6:02:02 PM","2020-03-21","Defect","Ship Staff","Ship Staff Insp.","# 1 Water Ballast Pump lower mechanical seal leaking","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.19","High","","","SEAL CHANGED & NO MORE LEAK OBSERVED","2020-06-20","","Completed","2020-04-07","No","No","No","Internal"]
[null,null,null,null,11196,"83_05-Apr-20 01:48:41","2020-03-27","Observation","Ship Staff","Ship Staff Insp.","MMC SHORE CALIBRATION CERTIFICATE EXPIRED","Hull & Tanks","Cargo / Ballast Systems","Equipment Related","8.25","Very High","","","SHORE REMOTE CALIBRATION CARRIED OUT & CERTIFICATE RECEIVED VIA EMAIL","2020-07-30","","Completed","2020-06-06","No","No","No","Internal"]
[null,null,null,null,null,"83_05-Apr-20 01:51:00","2020-03-27","Observation","Ship Staff","Ship Staff Insp.","Stevenson screen condition is poor and beyond repair.","Navigation - Others","Navigation","External Factors",8.24,"Medium","Not Applicable","Not Applicable","New stevenson screen received and put in place.","2020-06-28","ATHE200103","Completed","2020-10-26","No",null,null,"Internal"]
[null,null,null,null,null,"83_6/4/2020 7:07:47 AM","2020-04-05","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","220 volt alarm at many places. Need to replace light bulbs, fititng at many palces.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related",10.23,"Medium","Not Applicable","Not Applicable","Replaced bulb fittings","2020-09-20",null,"Completed","2020-09-10","No",null,null,"Internal"]
[null,null,null,null,null,"83_6/4/2020 6:54:24 AM","2020-04-05","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Soot collecting tank to fabricate for collecting / seperating soot.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","pipeline fabricated in dry dock","2020-09-05",null,"Completed","2020-10-27","No",null,null,"Internal"]
[null,null,null,null,null,"83_6/4/2020 6:48:40 AM","2020-04-05","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Lifeboat Davit hoisting Motor not able to take load while heaving. ","LSA / FFA","Safety / LSA / FFA","Equipment Related",5.1100000000000003,"Low","Not Applicable","Not Applicable","Shore technician attended the vessel in dry dock and overhauled the winch motor, all sheeves were made free by ship staff, lifeboat davit now fully functional.","2020-09-05",null,"Completed","2020-11-15","No",null,null,"Internal"]
[null,null,null,null,12113,"83_03-May-20 15:21:02","2020-04-06","Defect","Ship Staff","Ship Staff Insp.","Toilets flush of 2nd Officer cabin is supplying in-adequate water","Accommodation","General Appearance","Equipment Related","11.13","Low","","","Flush system inspected. Found vaccum air leak.  It has been rectified. Flush is working fine. No spare consumed.","2020-05-30","","Completed","2020-05-17","No","No","No","Internal"]
[null,null,null,null,12114,"83_6 Apr 2020 17:21:32","2020-04-06","Breakdown","Ship Staff","Ship Staff Insp.","No. 3 COP Suction gauge not working","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.25","Very High","","","RECEIVED NEW TRANSMITTER & FITTED.","2020-07-30","ATHE200021","Completed","2020-05-28","No","No","No","Internal"]
[null,null,null,null,null,"83_11-Jun-20 16:24:39","2020-04-10","Defect","Ship Staff","Ship Staff Insp.","Bridge AC unit not working","Navigation - Others","Navigation","Equipment Related",4.7,"High","Not Applicable","Not Applicable","Repaired by shore technician","2020-08-30",null,"Completed","2020-11-07","No",null,null,"Internal"]
[null,null,null,null,12109,"83_7/5/2020 9:51:03 PM","2020-04-20","Defect","Ship Staff","Ship Staff Insp.","# 2 D/G COOLING WATER PUMP IMPELLER FOUND DAMAGED WHEN OPENED UP FOR INSPECTION","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.31","Very High","","","DAMAGED IMPELLER RENEWED WITH NEW SPARE","2020-04-24","","Completed","2020-04-21","No","No","No","Internal"]
[null,null,null,null,12110,"83_7/5/2020 9:46:42 PM","2020-04-22","Defect","Ship Staff","Ship Staff Insp.","# 1 AUX BOILER FURNACE DOOR FOUND DAMAGED. ","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.31","Very High","","","SAME WAS FABRICATED & FITTED BACK","2020-04-25","","Completed","2020-04-22","No","No","No","Internal"]
[null,null,null,null,12111,"83_3/5/2020 11:52:56 PM","2020-04-25","Defect","Ship Staff","Ship Staff Insp.","# 2 Main Air Compressor, HP piston conrod Big End & Small End bearings found damaged. Same o'hauled with new bearing. Both LP piston conrod bearing renewal is also required, requisition raised for the same. ATHE200147","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related","10.31","Very High","","","Requisition raised ATHE200147","2020-07-25","","Completed","2020-04-25","No","No","No","Internal"]
[null,null,null,null,12112,"83_8/5/2020 9:27:46 AM","2020-04-27","Defect","Ship Staff","Ship Staff Insp.","# 1 E/R vent fan motor found making abnormal noise. Fan stopped immediately.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.31","Very High","","","Motor o'hauled with new bearings.","2020-04-30","","Completed","2020-04-28","No","No","No","Internal"]
[null,null,null,null,12115,"83_3 May 2020 16:49:26","2020-04-30","Defect,Observation","Ship Staff","Ship Staff Insp.","NO. 2  BALLAST PUMP UPPER MECH. SEAL LEAKING WHEN IN OPERATION.","Cargo Mach.,Deck - Machinery,Hull & Tanks","Cargo / Ballast Systems","Equipment Related","8.8","Medium","","","UPPER MECH. SEAL RENEWED & WBP TESTED.","2020-07-31","","Completed","2020-05-12","No","No","No","Internal"]
[null,null,null,null,null,"83_17-May-20 19:25:24","2020-05-12","Defect","Ship Staff","Ship Staff Insp.","Stbd Pump room Blower Fire Damper - the alignment ring for fire damper flap is broken from one side.","Deck - Machinery","Structural Condn. / WT integrity ","Equipment Related",8.4600000000000009,"Very High","Not Applicable","Not Applicable","Permanent repairs carried out in dry dock, new breaing and alingment ring put in place.","2020-09-17",null,"Completed","2020-10-24","Yes",null,null,"Internal"]
[null,null,null,null,13228,"83_18-Jun-20 09:47:00","2020-06-09","Observation","Ship Staff","Ship Staff Insp.","Aft Mooring winch M7 speed observed too slow while heaving.","Deck - Mooring Machinery","Mooring","Equipment Related","","","","","Speed Adjusted.","2020-06-20","","Completed","2020-06-15","No","No","No","Internal"]
[null,null,null,null,null,"83_29/6/2020 10:54:07 AM","2020-06-11","Defect","Ship Staff","Ship Staff Insp.","E/R # 2 vent fan motor burnt & also the fan blade is found broken.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related",10.31,"Very High","Not Applicable","Not Applicable","Renewed with new motor and fan","2020-08-01",null,"Completed","2020-10-25","No",null,null,"Internal"]
[null,null,null,null,13229,"83_8 Jul 2020 06:41:56","2020-06-26","Observation","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","The procedure for emergency opeation of Rescue boat davit was not posted locally","LSA / FFA","Safety / LSA / FFA","Human Error","5.3","Low","","","Procedure posted.","2020-07-31","","Completed","2020-06-26","No","No","No","External"]
[null,null,null,null,null,"83_8 Jul 2020 06:50:11","2020-06-26","Observation","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","The refractory for incenerator furnace back wall & door damaged at various locations","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","damaged refractory walls repaired with new refractory material","2020-07-31","ATHE200127","Completed","2020-09-20","No",null,null,"External"]
[null,null,null,null,null,"83_9/7/2020 1:07:27 PM","2020-06-26","Observation","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","Slight dent on the freefall Life boat rudder.","LSA / FFA","Safety / LSA / FFA","Equipment Related",8.69,"Medium","Not Applicable","Not Applicable","Repairs carried out during dry dock.","2020-09-26",null,"Completed","2020-10-24","No",null,null,"External"]
[null,null,null,null,null,"83_08-Jul-20 06:28:41","2020-06-26","Observation","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","Maintenance requirement for BWTS missing from PAL","Elect. Mach. & Equip.,Miscellaneous","Cargo / Ballast Systems","Equipment Related",6.22,"Medium","Not Applicable","Not Applicable","Maintenance requirement for BWTS added and updated in PAL","2020-07-31",null,"Completed","2020-10-19","No",null,null,"External"]
[null,null,null,null,null,"83_9/7/2020 1:02:38 PM","2020-06-26","Observation","SIRE / CDI Insp.","Others (Eg. Insurance etc.)","SWL mark for cranes hooks faded for Port midship crane & stbd provision.","Miscellaneous","General Appearance","Equipment Related",8.5,"Very High","Not Applicable","Not Applicable","SWL of the hooks stencilled.","2020-07-26",null,"Completed","2020-10-11","No",null,null,"External"]
[null,null,null,null,null,"83_2/9/2020 6:49:18 PM","2020-08-30","Defect","Ship Staff","Ship Staff Insp.","Hose handling crane ( S ) Boom up limit switch is not working found in stuck position","Deck - Machinery","Cargo / Ballast Systems","Equipment Related",8.5,"Very High","Not Applicable","Not Applicable","Limit switch removed & eased up, installed back but still not working. ","2020-11-30",null,"Completed","2020-11-22","No",null,null,"Internal"]
[null,null,null,null,null,"83_2/9/2020 6:56:28 PM","2020-08-30","Defect","Ship Staff","Ship Staff Insp.","Provision crane( Port ) limit switch cams for heaving up & lowering are damaged. Same needs renewal. Also both provision crane boom up limit switches found in stuck position & were found not working.","Deck - Machinery","Eng. / Strg. Comp.","Equipment Related",8.5,"Very High","Not Applicable","Not Applicable","LIMIT SWITCH REPLACED WITH RECEIVED SPARE ","2020-11-30",null,"Completed","2020-11-22","No",null,null,"Internal"]
[null,null,null,null,null,"83_24 Sep 2020 17:36:25","2020-09-15","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Poop deck saveall under mooring winch does not have drain plug.","Deck - Pipe / Fittings","Mooring","Human Error",null,null,"Not Applicable","Not Applicable","Drain plug put in place","2020-10-16",null,"Completed","2020-09-24","No",null,null,"Internal"]
[null,null,null,null,null,"83_24 Sep 2020 16:55:02","2020-09-16","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Fresh water filling pipe on poop deck did not have security seals","Deck - Pipe / Fittings","ISPS Related","Human Error",null,null,"Not Applicable","Not Applicable","Security seals put in place","2020-09-26",null,"Completed","2020-09-20","No",null,null,"Internal"]
[null,null,null,null,null,"83_24 Sep 2020 17:33:55","2020-09-16","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Liberian ensign flag was in damaged condition.","Miscellaneous","General Appearance","Human Error",null,null,"Not Applicable","Not Applicable","New flag was put in use.","2020-10-16",null,"Completed","2020-09-20","No",null,null,"Internal"]
[null,null,null,null,null,"83_24 Sep 2020 17:42:52","2020-09-16","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Gangway stencilling to be checked (max persons on lower and upper platforms)","Deck - Machinery,Miscellaneous","General Appearance","Behaviour Based",null,null,"Not Applicable","Not Applicable","Marking checked and same found as per manual.","2020-10-13",null,"Completed","2020-09-21","No",null,null,"Internal"]
[null,null,null,null,null,"83_24 Sep 2020 18:58:22","2020-09-16","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","\"B\" flag displayed on main mast was in poor condition, same to be renewed.","Miscellaneous","General Appearance","Human Error",null,null,"Not Applicable","Not Applicable","Flag renewed.","2020-10-16",null,"Completed","2020-09-20","No",null,null,"Internal"]
[null,null,null,null,null,"83_24/9/2020 22:53:09","2020-09-16","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Cylinder Oil measuring tank level gauge is gagged in open condition. This is serious observation as in case of the breakage of the sight glass - the oil may catch fire in case it comes into contact of source of ignition.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Human Error",10.25,"Very High","Not Applicable","Not Applicable","Gagged tool removed from place.Crew explained the consequence of keeping level gauge  in gagged position.","2020-09-17",null,"Completed","2020-09-16","No",null,null,"Internal"]
[null,null,null,null,null,"83_24/9/2020 22:56:17","2020-09-16","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ME unit #4 Fuel valve connection is leaking on the ME Cylinder Head.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related",10.29,"Medium","Not Applicable","Not Applicable","Leakage rectified by renewing gasket","2020-09-17",null,"Completed","2020-09-16","No",null,null,"Internal"]
[null,null,null,null,null,"83_24/9/2020 22:59:30","2020-09-16","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","#2 ME Fuel Oil Booster Pump relief valve has oil leak mark. This is to be rectified.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related",10.29,"Medium","Not Applicable","Not Applicable","bolts found slack,same tightened and leak arrested.","2020-09-18",null,"Completed","2020-09-17","No",null,null,"Internal"]
[null,null,null,null,null,"83_24/9/2020 23:12:04","2020-09-16","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","BWMS is in Alarm condition. This is to be investigated and rectified.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","system checked and alarm resetted.","2020-09-20",null,"Completed","2020-09-18","No",null,null,"Internal"]
[null,null,null,null,null,"83_24/9/2020 23:23:43","2020-09-16","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Aux Boiler Port side Steam Stop valve Gasket is leaking. To be replaced at first opportunity.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related",10.29,"Medium","Not Applicable","Not Applicable","packing replaced with new one,leak arrested.","2020-09-20",null,"Completed","2020-09-18","No",null,null,"Internal"]
[null,null,null,null,null,"83_24/9/2020 23:25:45","2020-09-16","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","EM Switch board 220V earth fault light for \"S\" and \"T\" Phase not lit. ","Critical Equip.","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Fused lamp replaced.","2020-09-17",null,"Completed","2020-09-16","No",null,null,"Internal"]
[null,null,null,null,null,"83_24 Sep 2020 17:40:21","2020-09-16","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ODME overboard valve number was not stencilled.","Miscellaneous","General Appearance","Human Error",null,null,"Not Applicable","Not Applicable","Stencilling done","2020-10-16",null,"Completed","2020-09-20","No",null,null,"Internal"]
[null,null,null,null,null,"83_24 Sep 2020 17:44:09","2020-09-16","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","One of the walkie talkie antenna was found to be damaged condition.","Miscellaneous","Communication","Behaviour Based",null,null,"Not Applicable","Not Applicable","Damaged antenna renewed","2020-10-16",null,"Completed","2020-09-22","No",null,null,"Internal"]
[null,null,null,null,null,"83_24 Sep 2020 18:30:00","2020-09-16","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","No 2 (P) & 3 (P)  WBT dome to be chipped and painted.","Miscellaneous","General Appearance","Human Error",null,null,"Not Applicable","Not Applicable","Derusting and painting carried out.","2020-10-15",null,"Completed","2020-10-21","No",null,null,"Internal"]
[null,null,null,null,null,"83_24 Sep 2020 18:41:17","2020-09-16","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Mooring winch remote operating stand hydraulic line supporting bracket is wasted.","Miscellaneous","General Appearance","Human Error",null,null,"Not Applicable","Not Applicable","Mooring winch remote control lines and fitting removed in dry dock.","2020-10-29",null,"Completed","2020-10-26","Yes",null,null,"Internal"]
[null,null,null,null,null,"83_24 Sep 2020 18:37:51","2020-09-16","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","No 2 COT fwd manhole to be derusted and painted","Miscellaneous","General Appearance","Human Error",null,null,"Not Applicable","Not Applicable","Derusting and painting carried out","2020-10-15",null,"Completed","2020-10-25","No",null,null,"Internal"]
[null,null,null,null,null,"83_24 Sep 2020 18:39:14","2020-09-16","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","No 2 (P) cargo tank bytterworth pocket fed manhole cover to be derusted and painted.","Miscellaneous","General Appearance","Human Error",null,null,"Not Applicable","Not Applicable","Derusting and painting carried out","2020-10-15",null,"Completed","2020-10-24","No",null,null,"Internal"]
[null,null,null,null,null,"83_24 Sep 2020 18:31:44","2020-09-16","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","3(P) PV valve to be checked for leak as strong smell was felt in the vicinity.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related",null,null,"Not Applicable","Not Applicable","All PV valves overhauled and pressure tested by shipyard.","2020-10-15",null,"Completed","2020-10-26","No",null,null,"Internal"]
[null,null,null,null,null,"83_24 Sep 2020 18:28:56","2020-09-16","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","No 3 (P) & 2 (P)  butterworth pocket manhole cover to be derusted and painted.","Miscellaneous","General Appearance","Human Error",null,null,"Not Applicable","Not Applicable","Derusting and painting carried out","2020-10-15",null,"Completed","2020-10-25","No",null,null,"Internal"]
[null,null,null,null,null,"83_24 Sep 2020 17:56:23","2020-09-16","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Bunker line last pressure testing date marked as Mar 2019","Miscellaneous","General Appearance","Behaviour Based",null,null,"Not Applicable","Not Applicable","Date marking is correct as it is for last 1.5 times MAWP which was done in Mar 2019","2020-10-15",null,"Completed","2020-09-20","No",null,null,"Internal"]
[null,null,null,null,null,"83_24 Sep 2020 18:56:48","2020-09-16","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Refrigerator in wheel house is not operational.","Miscellaneous","General Appearance","Equipment Related",null,null,"Not Applicable","Not Applicable","Troubleshooting carried out, refrigerator working satisfactorily now.","2020-10-30",null,"Completed","2020-09-25","No",null,null,"Internal"]
[null,null,null,null,null,"83_24 Sep 2020 18:33:16","2020-09-16","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","No 1(P),  2(P) and 3 (P) cargo tank dome to be chipped and painted.","Miscellaneous","General Appearance","Human Error",null,null,"Not Applicable","Not Applicable","Derusted and painted","2020-10-16",null,"Completed","2020-10-20","No",null,null,"Internal"]
[null,null,null,null,null,"83_24 Sep 2020 17:38:13","2020-09-16","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Poop deck saveall under mooring winch does not have drain plug.","Deck - Pipe / Fittings","Mooring","Human Error",null,null,"Not Applicable","Not Applicable","Drain plug put in place.","2020-10-15",null,"Completed","2020-09-24","No",null,null,"Internal"]
[null,null,null,null,null,"83_24 Sep 2020 16:57:06","2020-09-16","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Snap back zone - entire area to be marked as snap back zone, to erase existing markings around the mooring winch.","Miscellaneous","Mooring","Human Error",null,null,"Not Applicable","Not Applicable","Whole area is marked as snap back zone, no seperate marking done at mooring winches.","2020-10-16",null,"Completed","2020-10-10","No",null,null,"Internal"]
[null,null,null,null,null,"83_24/9/2020 23:03:17","2020-09-16","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","#1 Aux Boiler is in Alarm condition on the ECR Alarm monitoring system. This is to be investigated and rectified.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Problem resolved in alarm monitoring system","2020-09-30",null,"Completed","2020-09-28","No",null,null,"Internal"]
[null,null,null,null,null,"83_24/9/2020 23:05:27","2020-09-16","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ME Viscotherm is not operational.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Overhauling carried out with new spare","2020-09-30",null,"Completed","2020-10-01","No",null,null,"Internal"]
[null,null,null,null,null,"83_24/9/2020 23:09:23","2020-09-16","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Light Signal Column is in Alarm Condition. This is to be investigated and rectified.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Defective PCB  renewed with new spare","2020-10-05",null,"Completed","2020-09-30","No",null,null,"Internal"]
[null,null,null,null,null,"83_24/9/2020 23:15:40","2020-09-16","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","AMS DC PSU is in Alarm Condition. This is to be investigated and rectified.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Defective relay replaced with new one.","2020-10-05",null,"Completed","2020-09-26","No",null,null,"Internal"]
[null,null,null,null,null,"83_24/9/2020 23:07:18","2020-09-16","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","GE Viscotherm is not operational.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","working satisfactory.","2020-09-30",null,"Completed","2020-09-30","No",null,null,"Internal"]
[null,null,null,null,null,"83_24 Sep 2020 18:36:44","2020-09-16","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Morring wire hurdle (port side) for the breast winch needs chipping and painting","Miscellaneous","General Appearance","Human Error",null,null,"Not Applicable","Not Applicable","Derusted and painted.","2020-10-15",null,"Completed","2020-11-14","No",null,null,"Internal"]
[null,null,null,null,null,"83_24 Sep 2020 18:55:16","2020-09-16","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Split air conditioner in wheel house is not operational.","Navigation - Others","Navigation","Equipment Related",null,null,"Not Applicable","Not Applicable","Repaired by shore technician at Singapore","2020-10-30",null,"Completed","2020-11-07","No",null,null,"Internal"]
[null,null,null,null,null,"83_24 Sep 2020 18:42:10","2020-09-16","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Fwd mast top platform to be derusted and painted.","Miscellaneous","General Appearance","Human Error",null,null,"Not Applicable","Not Applicable","Fwd mast derusted and painted.","2020-10-14",null,"Completed","2020-12-03","No",null,null,"Internal"]
[null,null,null,null,null,"83_24 Sep 2020 18:16:54","2020-09-16","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","No 2 cargo line on port side has rust pitting mark.","Miscellaneous","General Appearance","Human Error",null,null,"Not Applicable","Not Applicable","Derusted and painted","2020-10-16",null,"Completed","2020-12-18","No",null,null,"Internal"]
[null,null,null,null,null,"83_24 Sep 2020 17:45:50","2020-09-16","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Diesel oil line pressure guage socket badly rusted.","Miscellaneous","General Appearance","Behaviour Based",null,null,"Not Applicable","Not Applicable","Derusted and painted","2020-10-15",null,"Completed","2020-12-18","No",null,null,"Internal"]
[null,null,null,null,null,"83_24 Sep 2020 18:26:07","2020-09-16","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","No 3 (P0 and 2(P) WB tank manhole cover port to be chipped and painted.","Miscellaneous","General Appearance","Human Error",null,null,"Not Applicable","Not Applicable","Derusted and painted","2020-10-15",null,"Completed","2020-12-18","No",null,null,"Internal"]
[null,null,null,null,null,"83_24 Sep 2020 18:27:36","2020-09-16","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","40T double bollard fwd of manifold to be chipped and painted.","Deck - Pipe / Fittings","General Appearance","Human Error",null,null,"Not Applicable","Not Applicable","Derusted and painted","2020-10-15",null,"Completed","2020-12-18","No",null,null,"Internal"]
[null,null,null,null,null,"83_24 Sep 2020 16:59:29","2020-09-16","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Mooring winch brakes - Brake liner adjustment bolts needs to be adjusted to maintain uniform gap.","Deck - Machinery","Mooring","Human Error",null,null,"Not Applicable","Not Applicable","Adjusting bolts checked and adjusted.","2020-10-16",null,"Completed","2020-12-18","No",null,null,"Internal"]
[null,null,null,null,null,"83_24/11/2020 18:43:06","2020-11-07","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ME exhaust valve no:6 to overhaul","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related",10.29,"Medium","Not Applicable","Not Applicable","Replaced with overhauled one.","2020-11-30",null,"Completed","2020-11-17","No",null,null,"Internal"]
[null,null,null,null,null,"83_23 Nov 2020 19:14:45","2020-11-23","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Officer Changing Room and Crew Changing Room is Dirty. This needs to be tidied up","Miscellaneous","General Appearance","Behaviour Based",null,null,"Not Applicable","Not Applicable","Changing rooms squared up","2020-11-25",null,"Completed","2020-11-23","No",null,null,"Internal"]
[null,null,null,null,null,"83_23 Nov 2020 19:16:35","2020-11-23","Critical Equipment","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Lifeboat davit sheave to be made free and davit RAM PIN to be greased","LSA / FFA","Safety / LSA / FFA","Equipment Related",null,null,"Not Applicable","Not Applicable","Lifeboat davit sheeves made free and greasing of davit RAM carried out.","2020-11-30",null,"Completed","2020-11-23","No",null,null,"Internal"]
[null,null,null,null,null,"83_24/11/2020 14:37:45","2020-11-23","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","LT cooler temp.controller area and pipeline to be cleaned.","E/R - Aux. Mach.","Eng. / Strg. Comp.","External Factors",10.32,"Very High","Not Applicable","Not Applicable","Cleaning carried out.","2020-11-30",null,"Completed","2020-11-25","No",null,null,"Internal"]
[null,null,null,null,null,"83_24/11/2020 14:50:17","2020-11-23","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Comp.boiler manhole door to be cleaned and painted.","E/R - Boiler","Eng. / Strg. Comp.","Human Error",10.32,"Very High","Not Applicable","Not Applicable","Cleaned and painted.","2020-11-30",null,"Completed","2020-11-25","No",null,null,"Internal"]
[null,null,null,null,null,"83_24/11/2020 17:39:48","2020-11-23","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Composite boiler steam stop valve leakage to rectify","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Gland packing renewed and leakage arrested.","2020-11-30",null,"Completed","2020-11-23","No",null,null,"Internal"]
[null,null,null,null,null,"83_24/11/2020 18:38:42","2020-11-23","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Upper deck MCP near starboard side door is hanging","Elect. Mach. & Equip.","Emgcy. Systems","Human Error",10.37,"Medium","Not Applicable","Not Applicable","Fixed in place","2020-11-30",null,"Completed","2020-11-25","No",null,null,"Internal"]
[null,null,null,null,null,"83_24-Nov-20 19:12:10","2020-11-23","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","GMDSS Logbook entry for L/B radio weekly test not entered in record of GMDSS equipment test section.","Navigation - GMDSS & Communication","Communication","Human Error",null,null,"Not Applicable","Not Applicable","Regular entriesare now being made for L/B radio weekly test routine in GMDSS record book.","2020-11-30",null,"Completed","2020-11-24","No",null,null,"Internal"]
[null,null,null,null,null,"83_24-Nov-20 19:13:46","2020-11-23","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Drills conducted on 06 Nov 2020 not entered in the deck logbook.","Documentation","Cert. & Docu.","Human Error",null,null,"Not Applicable","Not Applicable","Completed Pending entries in Deck Logbook for the Drills conducted of 06th November 2020.","2020-11-30",null,"Completed","2020-11-24","No",null,null,"Internal"]
[null,null,null,null,null,"83_24-Nov-20 19:16:03","2020-11-23","Non Conformity","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Water ingress alarm panel for Fwd void Space, Bosun Store and Bow Thruster room was noted to be powered down. Same to be investigated and made operational.","Miscellaneous","Cargo / Ballast Systems","Human Error",null,null,"Not Applicable","Not Applicable","Water Ingress alarm system is operational.","2020-11-30",null,"Completed","2020-11-24","No",null,null,"Internal"]
[null,null,null,null,null,"83_24-Nov-20 19:17:57","2020-11-23","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Non WGS - 84 chart at EOPL not considered as part of the passgae plan.","Navigation - ECDIS","Navigation","Human Error",null,null,"Not Applicable","Not Applicable","Non WGS 84 cells in the vicinty of the route will be considered and notify/caution all Naviagting officers during Pasage Plan meeting. ","2020-11-30",null,"Completed","2020-11-24","No",null,null,"Internal"]
[null,null,null,null,null,"83_24-Nov-20 19:23:51","2020-11-23","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Gas Alarm repeater panel on the bridge was noted to be powered down. Same to be investigated ","Miscellaneous","Cargo / Ballast Systems","Human Error",null,null,"Not Applicable","Not Applicable","Gas detection system switched on.","2020-11-30",null,"Completed","2020-11-24","No",null,null,"Internal"]
[null,null,null,null,null,"83_24/11/2020 14:26:08","2020-11-23","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","AE#1 Air cooler cover to be cleaned and painted.","E/R - Aux. Engine","Eng. / Strg. Comp.","External Factors",10.29,"Medium","Not Applicable","Not Applicable"," cleaned and painted.","2020-12-10",null,"Completed","2020-11-26","No",null,null,"Internal"]
[null,null,null,null,null,"83_24/11/2020 14:29:32","2020-11-23","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Newly fabricated electrical cable stand(near Aux.air reservoir) to be primered and painted.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","External Factors",10.29,"Medium","Not Applicable","Not Applicable","Priming done and painted","2020-11-30",null,"Completed","2020-11-27","No",null,null,"Internal"]
[null,null,null,null,null,"83_24/11/2020 14:34:05","2020-11-23","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Emergency Air bottle and adjoining area has soot deposit mark.","E/R - Aux. Mach.","Eng. / Strg. Comp.","External Factors",10.29,"Medium","Not Applicable","Not Applicable"," cleaned and painted.","2020-11-30",null,"Completed","2020-11-27","No",null,null,"Internal"]
[null,null,null,null,null,"83_24/11/2020 14:45:00","2020-11-23","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Air vent Trunk aft of ME manouvering platform needs cleaning.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","External Factors",10.29,"Medium","Not Applicable","Not Applicable","Cleaning carried out","2020-11-30",null,"Completed","2020-11-27","No",null,null,"Internal"]
[null,null,null,null,null,"83_24/11/2020 14:46:59","2020-11-23","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Vacuum condenser end cover area to be cleaned and painted.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","External Factors",10.29,"Medium","Not Applicable","Not Applicable","Cleaning done and painted.","2020-11-30",null,"Completed","2020-11-25","No",null,null,"Internal"]
[null,null,null,null,null,"83_24/11/2020 17:41:48","2020-11-23","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Aux.boiler 1&2 furnace door cleaning and painting","E/R - Boiler","Eng. / Strg. Comp.","Human Error",10.29,"Medium","Not Applicable","Not Applicable","Cleaning done and painted.","2020-11-30",null,"Completed","2020-11-25","No",null,null,"Internal"]
[null,null,null,null,null,"83_24/11/2020 18:35:45","2020-11-23","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","IG fan and motor to be cleaned.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Human Error",10.29,"Medium","Not Applicable","Not Applicable","Cleaning carried out.","2020-11-30",null,"Completed","2020-11-28","No",null,null,"Internal"]
[null,null,null,null,null,"83_28/11/2020 13:58:06","2020-11-23","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Boiler gauge glass LED(3 No.s) not working","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related",10.31,"Very High","Not Applicable","Not Applicable","Renewed with spare one,made operational","2020-11-30",null,"Completed","2020-11-27","No",null,null,"Internal"]
[null,null,null,null,null,"83_23 Nov 2020 19:04:34","2020-11-23","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","IG fresh air intake blank packing to be renewed.","Inert Gas","General Appearance","External Factors",null,null,"Not Applicable","Not Applicable","Packing renewed.","2020-12-20",null,"Completed","2020-11-27","No",null,null,"Internal"]
[null,null,null,null,null,"83_23 Nov 2020 19:09:20","2020-11-23","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Many loose and heavy items are stowed in bulldozer parking area, same to be cleared / secured.","Miscellaneous","General Appearance","Behaviour Based",null,null,"Not Applicable","Not Applicable","Blldozer parking area cleared / secured.","2020-12-20",null,"Completed","2020-11-28","No",null,null,"Internal"]
[null,null,null,null,null,"83_24 Nov 2020 18:11:06","2020-11-23","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Numerous new fittings on main deck from recently completed docking noted not painted.","Miscellaneous","General Appearance","External Factors",null,null,"Not Applicable","Not Applicable","New fittings buffed and painted.","2020-12-20",null,"Completed","2020-11-30","No",null,null,"Internal"]
[null,null,null,null,null,"83_24/11/2020 14:22:32","2020-11-23","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","LSMGO cooler plate for DG and boiler to be cleaned.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Plate cleaned and tried out,working satisfactory.","2020-12-10",null,"Completed","2020-11-30","No",null,null,"Internal"]
[null,null,null,null,null,"83_24/11/2020 17:34:27","2020-11-23","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Composite boiler drip tray to be cleaned and painted.","E/R - Boiler","Eng. / Strg. Comp.","Human Error",10.29,"Medium","Not Applicable","Not Applicable","Cleaned and painted.","2020-11-30",null,"Completed","2020-11-29","No",null,null,"Internal"]
[null,null,null,null,null,"83_24/11/2020 17:36:57","2020-11-23","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Ultrasonic cleaning machine to be installed","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Human Error",10.32,"Very High","Not Applicable","Not Applicable","installion done.","2020-12-15",null,"Completed","2020-12-01","No",null,null,"Internal"]
[null,null,null,null,null,"83_23 Nov 2020 19:07:00","2020-11-23","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Port side rescue boat deck top coat is eroding and base layer is visible, area to be recoated.","Miscellaneous","General Appearance","External Factors",null,null,"Not Applicable","Not Applicable","Affected area, fresh water washed and recoated.","2021-04-15",null,"Completed","2020-12-23","No",null,null,"Internal"]
[null,null,null,null,null,"83_2/1/2021 22:53:59","2020-12-30","Observation","Ship Staff","Ship Staff Insp.","AE#1 High temperature cooling water pump mechanical seal leaking","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Mechanical seal renewed.","2020-12-31",null,"Completed","2020-12-30","No",null,null,"Internal"]

{"sheet":"Calc","index":2,"n_rows":28,"n_cols":12,"rows_kept":28,"cut":false,"hidden":true,"merged":[]}
["Def_type","Def_cause","Equipments","VIQrefno","Observer_code"]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,"Dim itemSele As Long"]
[null,null,null,null,null,null,null,null,null,null,null,"   dim startRow as integer"]
[null,null,null,null,null,null,null,null,null,null,null,"   startRow=1"]
[null,null,null,null,null,null,null,null,null,null,null,"        For itemSele = 0 To ListBox1.ListCount - 1"]
[null,null,null,null,null,null,null,null,null,null,null,"        If ListBox1.Selected(itemSele) = True Then"]
[null,null,null,null,null,null,null,null,null,null,null,"        Worksheets(\"WorksheetName\").Range(\"A\" & startRow).Value = ListBox1.List(itemSele)"]
[null,null,null,null,null,null,null,null,null,null,null,"        startRow = startRow + 1"]
[null,null,null,null,null,null,null,null,null,null,null,"        End If"]
[null,null,null,null,null,null,null,null,null,null,null,"        Next"]
[null,null,null,null,null,null,null,null,null,null,null,"Dim LastRowA As String"]
[null,null,null,null,null,null,null,null,null,null,null,"        Dim itemSele As Long"]
[null,null,null,null,null,null,null,null,null,null,null,"       Dim startRow as integer"]
[null,null,null,null,null,null,null,null,null,null,null,"        LastRowA = ActiveSheet.Cells(Rows.count, \"A\").End(xlUp).row"]
[null,null,null,null,null,null,null,null,null,null,null,"        startQue = 0"]
[null,null,null,null,null,null,null,null,null,null,null,"        For itemSele = 0 To ListBox1.ListCount - 1"]
[null,null,null,null,null,null,null,null,null,null,null,"        For startRow = 1 To LastRowA"]
[null,null,null,null,null,null,null,null,null,null,null,"        If Worksheets(\"WorksheetName\").Range(\"A\" & startRow).Value = ListBox1.List(itemSele) Then"]
[null,null,null,null,null,null,null,null,null,null,null,"        ListBox1.Selected(itemSele) = True"]
[null,null,null,null,null,null,null,null,null,null,null,"        Exit For"]
[null,null,null,null,null,null,null,null,null,null,null,"        End If"]
[null,null,null,null,null,null,null,null,null,null,null,"        Next j"]
[null,null,null,null,null,null,null,null,null,null,null,"        Next"]
[null,null,null,null,null,null,null,null,null,null,null,"        End If"]

{"sheet":"Areaofobs","index":3,"n_rows":17,"n_cols":2,"rows_kept":17,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Cargo / Ballast Systems",11]
["Cert. & Docu.",2]
["Communication",6]
["Crew Management",3]
["Emgcy. Systems",13]
["Eng. / Strg. Comp.",14]
["General Appearance",15]
["Ice Opns.",17]
["ISM Related",7]
["ISPS Related",10]
["MARPOL Related",9]
["MLC Related",4]
["Mooring",12]
["Navigation",5]
["Safety / LSA / FFA",8]
["Structural Condn. / WT integrity ",16]

{"sheet":"Vessel_type","index":4,"n_rows":1,"n_cols":2,"rows_kept":1,"cut":false,"hidden":true,"merged":[]}
["Vessel_type","ID"]

{"sheet":"Deficiency_type","index":5,"n_rows":8,"n_cols":3,"rows_kept":8,"cut":false,"hidden":true,"merged":[]}
["TITLE","Type of deficiency_description","ID"]
["Breakdown",null,6]
["Critical Equipment",null,4]
["Defect",null,1]
["Guarantee Claim",null,8]
["Non Conformity",null,2]
["Observation",null,3]
["Other",null,7]

{"sheet":"VIQrefno","index":6,"n_rows":427,"n_cols":3,"rows_kept":427,"cut":false,"hidden":true,"merged":[]}
["VIQ_ref_no","Risk Value of observation","ID"]
["1.1","Low",8243]
["1.10","Low",8252]
["1.11","Low",8253]
["1.12","Low",8254]
["1.13","Low",8255]
["1.14","Low",8256]
["1.15","Low",8257]
["1.16","Low",8259]
["1.17","Low",8260]
["1.18","Low",8261]
["1.19","Low",8262]
["1.2","Low",8244]
["1.20","Low",8263]
["1.21","Low",8265]
["1.22","Low",8266]
["1.23","Low",8267]
["1.24","Low",8268]
["1.25","Low",8269]
["1.26","Low",8270]
["1.3","Low",8245]
["1.4","Low",8246]
["1.5","Low",8247]
["1.6","Low",8248]
["1.7","Low",8249]
["1.8","Low",8250]
["1.9","Low",8251]
["1.99","High",11258]
["10.1","Medium",8461]
["10.10","High",8470]
["10.11","Medium",8471]
["10.12","Very High",8472]
["10.13","Very High",8473]
["10.14","Medium",8474]
["10.15","Low",8475]
["10.16","Very High",8476]
["10.17","Very High",8477]
["10.18","High",8478]
["10.19","Very High",8479]
["10.2","Low",8462]
["10.20","High",8480]
["10.21","Medium",8481]
["10.22","Low",8482]
["10.23","Medium",8483]
["10.24","Low",8484]
["10.25","Very High",8485]
["10.26","High",8486]
["10.27","Medium",8487]
["10.28","Low",8488]
["10.29","Medium",8489]
["10.3","Medium",8463]
["10.30","High",8490]
["10.31","Very High",8491]
["10.32","Very High",8492]
["10.33","High",8493]
["10.34","High",8494]
["10.35","Very High",8495]
["10.36","Very High",8496]
["10.37","Medium",8497]
["10.38","Medium",8498]
["10.39","High",8499]
["10.4","High",8464]
["10.40","Medium",8500]
["10.41","Medium",8501]
["10.42","Medium",8502]
["10.43","Medium",8503]
["10.44","Medium",8504]
["10.45","Very High",8505]
["10.46","High",8506]
["10.47","Medium",8507]
["10.48","High",8508]
["10.49","Medium",8509]
["10.5","Low",8465]
["10.50","High",8510]
["10.51","Low",8511]
["10.52","Medium",8512]
["10.53","Medium",8513]
["10.54","High",8514]
["10.55","Low",8515]
["10.6","Very High",8466]
["10.7","Medium",8467]
["10.8","Medium",8468]
["10.9","Medium",8469]
["10.99","High",8516]
["11.1","High",8420]
["11.10","Medium",8429]
["11.11","Very High",8430]
["11.12","Low",8431]
["11.13","Low",8432]
["11.14","Medium",8433]
["11.15","Low",8434]
["11.16","Low",8435]
["11.17","Low",8436]
["11.2","Medium",8421]
["11.3","Medium",8422]
["11.4","Very High",8423]
["11.5","Medium",8424]
["11.6","Medium",8425]
["11.7","High",8426]
["11.8","Low",8427]
["11.9","Low",8428]
["11.99","High",8437]
["12.1","High",8438]
["12.10","High",8448]
["12.11","High",8449]
["12.12","High",8450]
["12.13","High",8451]
["12.14","High",8452]
["12.15","High",8453]
["12.16","High",8454]
["12.17","High",8455]
["12.18","High",8456]
["12.19","High",8457]
["12.2","High",8439]
["12.20","High",8458]
["12.21","High",8459]
["12.3","High",8441]
["12.4","High",8442]
["12.5","High",8443]
["12.6","High",8444]
["12.7","High",8445]
["12.8","High",8446]
["12.9","High",8447]
["12.99","High",8460]
["2.1","Very High",8296]
["2.1.9","Very High",11259]
["2.10","Medium",8304]
["2.11","Medium",8305]
["2.12","Low",8306]
["2.13","Low",8307]
["2.14","Low",8308]
["2.15","Low",8309]
["2.16","Medium",8310]
["2.2","Medium",8297]
["2.3","High",8295]
["2.4","Medium",8298]
["2.5","Medium",8299]
["2.6","Low",8300]
["2.7","High",8301]
["2.8","High",8302]
["2.9","Medium",8303]
["2.99","High",8311]
["3.1","High",8312]
["3.2","Very High",8313]
["3.3","High",8314]
["3.4","Low",8294]
["3.5","Medium",8315]
["3.6","High",8316]
["3.7","Very High",8317]
["3.8","Very High",8318]
["3.99","High",8319]
["4.1","High",8320]
["4.10","High",8329]
["4.11","Medium",8330]
["4.12","Very High",8331]
["4.13","Very High",8332]
["4.14","Very High",8333]
["4.15","Very High",8334]
["4.16","Very High",8335]
["4.17","Very High",8336]
["4.18","Very High",8337]
["4.19","Low",8338]
["4.2","Medium",8321]
["4.20","Very High",8339]
["4.21","High",8340]
["4.22","Low",8341]
["4.23","High",8342]
["4.24","High",8343]
["4.25","Low",8344]
["4.26","Low",8345]
["4.27","High",8346]
["4.3","Medium",8322]
["4.4","High",8323]
["4.5","Very High",8324]
["4.6","Medium",8325]
["4.7","High",8326]
["4.8","Medium",8327]
["4.9","Medium",8328]
["4.99","High",8347]
["5.1","Very High",8517]
["5.10","High",8526]
["5.11","Low",8527]
["5.12","Medium",8528]
["5.13","High",8529]
["5.14","Very High",8530]
["5.15","Medium",8531]
["5.16","Very High",8532]
["5.17","Very High",8533]
["5.18","High",8534]
["5.19","Medium",8535]
["5.2","Very High",8518]
["5.20","Medium",8536]
["5.21","Medium",8537]
["5.22","High",8539]
["5.23","Very High",8540]
["5.24","Very High",8541]
["5.25","Medium",8542]
["5.26","Medium",8543]
["5.27","Medium",8544]
["5.28","Very High",8545]
["5.29","High",8546]
["5.3","Low",8519]
["5.30","High",8547]
["5.31","High",8548]
["5.32","High",8549]
["5.33","High",8550]
["5.34","Low",8551]
["5.35","Medium",8552]
["5.36","Low",8553]
["5.37","Low",8554]
["5.38","High",8555]
["5.39","Very High",8556]
["5.4","High",8520]
["5.40","Very High",8557]
["5.41","Very High",8558]
["5.42","Medium",8559]
["5.43","High",8560]
["5.44","High",8561]
["5.45","Medium",8564]
["5.46","Medium",8565]
["5.47","Medium",8566]
["5.48","Medium",8567]
["5.5","Low",8521]
["5.6","Low",8522]
["5.7","Medium",8523]
["5.8","Medium",8524]
["5.9","Very High",8525]
["5.99","High",8568]
["6.1","Medium",8348]
["6.10","Low",8357]
["6.11","High",8358]
["6.12","Medium",8359]
["6.13","Low",8360]
["6.14","High",8361]
["6.15","High",8362]
["6.16","Very High",8363]
["6.17","Very High",8364]
["6.18","Medium",8365]
["6.19","Low",8366]
["6.2","High",8349]
["6.20","Medium",8367]
["6.21","High",8368]
["6.22","Medium",8369]
["6.3","Low",8350]
["6.4","High",8351]
["6.5","Medium",8352]
["6.6","Medium",8353]
["6.7","High",8354]
["6.8","High",8355]
["6.9","Low",8356]
["6.99","High",8370]
["7.1","High",8371]
["7.10","High",8380]
["7.11","High",8381]
["7.12","High",8382]
["7.13","Medium",8383]
["7.14","Medium",8384]
["7.15","High",8385]
["7.16","High",8386]
["7.17","High",8387]
["7.2","High",8372]
["7.3","Low",8373]
["7.4","Low",8374]
["7.5","Low",8375]
["7.6","Medium",8376]
["7.7","Low",8377]
["7.8","High",8378]
["7.9","High",8379]
["7.99","High",8388]
["8.1","Very High",8569]
["8.10","Very High",8578]
["8.100","Low",11227]
["8.101","Medium",11228]
["8.102","Low",11229]
["8.103","Low",11230]
["8.104","Low",11231]
["8.105","Medium",11232]
["8.106","Medium",11233]
["8.107","Low",11234]
["8.108","High",11235]
["8.109","Very High",11236]
["8.11","Medium",8579]
["8.110","High",11237]
["8.111","Medium",11238]
["8.112","High",11239]
["8.113","Medium",11240]
["8.114","Low",11241]
["8.115","High",11242]
["8.116","Medium",11243]
["8.117","Medium",11244]
["8.118","Medium",11245]
["8.119","High",11246]
["8.12","Medium",8580]
["8.120","High",11247]
["8.121","Medium",11248]
["8.122","High",11249]
["8.123","High",11250]
["8.124","Low",11251]
["8.125","High",11252]
["8.126","Medium",11253]
["8.127","Medium",11254]
["8.13","Medium",8581]
["8.14","Very High",8582]
["8.15","High",8583]
["8.16","Very High",8584]
["8.17","Low",8585]
["8.18","High",8586]
["8.19","High",8587]
["8.199","High",11255]
["8.2","Medium",8570]
["8.20","Medium",8588]
["8.21","High",8589]
["8.22","Very High",8590]
["8.23","Medium",8591]
["8.24","Medium",8592]
["8.25","Very High",8593]
["8.26","High",8594]
["8.27","Medium",8595]
["8.28","Medium",8596]
["8.29","High",8598]
["8.3","Very High",8571]
["8.30","High",8599]
["8.31","High",8600]
["8.32","Low",8601]
["8.33","Medium",8602]
["8.34","High",8603]
["8.35","Medium",8604]
["8.36","Medium",8605]
["8.37","High",8607]
["8.38","Medium",8608]
["8.39","Medium",8609]
["8.4","Medium",8572]
["8.40","High",8610]
["8.41","Medium",8611]
["8.42","Medium",8612]
["8.43","Very High",8613]
["8.44","High",8615]
["8.45","High",8616]
["8.46","Very High",8617]
["8.47","Very High",8618]
["8.48","Medium",8619]
["8.49","High",8620]
["8.5","Very High",8573]
["8.50","Medium",8621]
["8.51","Low",8622]
["8.52","Low",8623]
["8.53","Low",8624]
["8.54","High",8625]
["8.55","Low",11182]
["8.56","Medium",11183]
["8.57","Medium",11184]
["8.58","High",11185]
["8.59","High",11186]
["8.6","Medium",8574]
["8.60","High",11187]
["8.61","Medium",11188]
["8.62","Very High",11189]
["8.63","High",11190]
["8.64","Medium",11191]
["8.65","Low",11192]
["8.66","High",11193]
["8.67","High",11194]
["8.68","High",11195]
["8.69","Medium",11196]
["8.7","High",8575]
["8.70","Medium",11197]
["8.71","Very High",11198]
["8.72","Medium",11199]
["8.73","Medium",11200]
["8.74","High",11201]
["8.75","Medium",11202]
["8.76","Medium",11203]
["8.77","Medium",11204]
["8.78","Medium",11205]
["8.79","Medium",11206]
["8.8","Medium",8576]
["8.80","Medium",11207]
["8.81","Low",11208]
["8.82","Medium",11209]
["8.83","Low",11210]
["8.84","Low",11211]
["8.85","Medium",11212]
["8.86","Medium",11213]
["8.87","Medium",11214]
["8.88","Low",11215]
["8.89","High",11216]
["8.9","High",8577]
["8.90","High",11217]
["8.91","High",11218]
["8.92","Medium",11219]
["8.93","Low",11220]
["8.94","Low",11221]
["8.95","Medium",11222]
["8.96","Medium",11223]
["8.97","Low",11224]
["8.98","High",11225]
["8.99","Medium",11226]
["9.1","Low",8390]
["9.10","Medium",8399]
["9.11","Medium",8400]
["9.12","Medium",8401]
["9.13","Low",8402]
["9.14","Medium",8403]
["9.15","Medium",8404]
["9.16","High",8405]
["9.17","High",8406]
["9.18","Low",8407]
["9.19","Low",8408]
["9.2","Very High",8391]
["9.20","Medium",8409]
["9.21","Medium",8410]
["9.22","Low",8411]
["9.23","Low",8412]
["9.24","Medium",8413]
["9.25","Low",8414]
["9.26","Low",8415]
["9.27","Low",8416]
["9.28","Medium",8417]
["9.29","Low",8418]
["9.3","Very High",8392]
["9.4","High",8393]
["9.5","High",8394]
["9.6","Low",8395]
["9.7","Medium",8396]
["9.8","Medium",8397]
["9.9","Medium",8398]
["9.99","High",8419]

{"sheet":"Equipment_list","index":7,"n_rows":28,"n_cols":3,"rows_kept":28,"cut":false,"hidden":true,"merged":[]}
["TITLE","Equipment_list_description","ID"]
["Accommodation",null,12]
["Cargo Mach.",null,13]
["Critical Equip.",null,16]
["Deck - Machinery",null,18]
["Deck - Mooring Machinery",null,15]
["Deck - Pipe / Fittings",null,20]
["Documentation",null,21]
["E/R - Air Comp.",null,8]
["E/R - Aux. Engine",null,4]
["E/R - Aux. Mach.",null,7]
["E/R - Boiler",null,5]
["E/R - Main Engine",null,3]
["E/R - Pipes/ valves & fittings",null,9]
["E/R - Pumps",null,32]
["E/R - Purifier",null,6]
["Elect. Mach. & Equip.",null,10]
["Hull & Tanks",null,19]
["Inert Gas",null,14]
["LSA / FFA",null,17]
["Miscellaneous",null,22]
["Navigation - DGPS / EPFS / AIS",null,28]
["Navigation - ECDIS",null,25]
["Navigation - Echo Sounder / Speed Log",null,26]
["Navigation - GMDSS & Communication",null,23]
["Navigation - Others",null,11]
["Navigation - RADAR",null,24]
["Navigation - VDR / BNWAS",null,30]

{"sheet":"PSC_MOU","index":8,"n_rows":11,"n_cols":3,"rows_kept":11,"cut":false,"hidden":true,"merged":[]}
["TITLE","PSC_MOU_description","ID"]
["Asia and the Pacific",null,2]
["Caribbean",null,4]
["Europe and the North Atlantic",null,1]
["Latin America",null,3]
["The Black Sea region",null,6]
["The Indian Ocean",null,8]
["The Mediterranean",null,7]
["The Riyadh MoU",null,9]
["USCG",null,10]
["West and Central Africa",null,5]

{"sheet":"Inspection_type","index":9,"n_rows":13,"n_cols":2,"rows_kept":13,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Bunkering Audit",14]
["Cargo Audit",17]
["Engineering Audit",16]
["ISM Audit",2]
["ISPS Audit",3]
["IT Audit",10]
["MLC Audit",1]
["Mooring Audit",9]
["Nav Audit / Verification",8]
["Onboard Training",18]
["Ship Staff Insp.",15]
["Suptd. Insp.",13]

{"sheet":"Deficiency_Cause","index":10,"n_rows":8,"n_cols":3,"rows_kept":8,"cut":false,"hidden":true,"merged":[]}
["TITLE","Deficiency_Cause_description","ID"]
["Behaviour Based",null,1]
["Equipment Related",null,4]
["External Factors",null,5]
["Human Error",null,7]
["Inappropriate Procedure",null,8]
["Industry Issue",null,6]
["Knowledge Based",null,3]

{"sheet":"Observer_code","index":11,"n_rows":3,"n_cols":3,"rows_kept":3,"cut":false,"hidden":true,"merged":[]}
["TITLE","Observer_code_description","ID"]
["Owner / Marine / Tech. Suptd.",null,3]
["Ship Staff",null,2]

{"sheet":"Status_code","index":12,"n_rows":8,"n_cols":3,"rows_kept":8,"cut":false,"hidden":true,"merged":[]}
["TITLE","Status_code_description","ID"]
[]
["Completed",null,6]
["Deferred to D D",null,5]
["In progress",null,3]
["Not Started",null,2]
["Waiting spare",null,4]
["xyz",null,8]

{"sheet":"PSC_ref_no","index":13,"n_rows":19,"n_cols":2,"rows_kept":19,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Alarms",9]
["Cargo operations including equipment",7]
["Certificates & Documentation",2]
["Dangerous Goods",13]
["Emergency Systems",5]
["Fire safety",8]
["ISM",16]
["ISPS",17]
["Life saving appliances",12]
["MLC, 2006",18]
["Other",19]
["Pollution Prevention",15]
["Propulsion and auxiliary machinery",14]
["Radio communication",6]
["Safety of Navigation",11]
["Structural condition",3]
["Water/Weathertight condition",4]
["Working and Living Conditions",10]

{"sheet":"Risk_value_of_obs","index":14,"n_rows":1,"n_cols":2,"rows_kept":1,"cut":false,"hidden":true,"merged":[]}
["Risk Value of observation","ID"]

{"sheet":"Year","index":15,"n_rows":18,"n_cols":1,"rows_kept":18,"cut":false,"hidden":true,"merged":[]}
["Year"]
[2014]
[2015]
[2016]
[2017]
[2018]
[2019]
[2020]
[2021]
[2022]
[2023]
[2024]
[2025]
[2026]
[2027]
[2028]
[2029]
[2030]

{"sheet":"Month","index":16,"n_rows":13,"n_cols":1,"rows_kept":13,"cut":false,"hidden":true,"merged":[]}
["Month"]
["Jan"]
["Feb"]
["Mar"]
["Apr"]
["May"]
["Jun"]
["Jul"]
["Aug"]
["Sep"]
["Oct"]
["Nov"]
["Dec"]

{"sheet":"Date_","index":17,"n_rows":32,"n_cols":1,"rows_kept":32,"cut":false,"hidden":true,"merged":[]}
["Date"]
["01"]
["02"]
["03"]
["04"]
["05"]
["06"]
["07"]
["08"]
["09"]
[10]
[11]
[12]
[13]
[14]
[15]
[16]
[17]
[18]
[19]
[20]
[21]
[22]
[23]
[24]
[25]
[26]
[27]
[28]
[29]
[30]
[31]

{"sheet":"Sheet1","index":18,"n_rows":24,"n_cols":6,"rows_kept":24,"cut":false,"hidden":true,"merged":[]}
[]
[null,"ID","E",null,"Date Recorded",1]
[null,"UNIQUE ID","F",null,"Type of Deficiency",2]
[1,"Date Recorded","G",null,"Observer code",3]
["ignore","Vessel Type","H",null,"Type of Inspection",4]
[null,"Internal / External","I",null,"Description of Deficiency",5]
[null,"Drydock","J",null,"Equipment Categories",6]
[null,"Information Sharing","K",null,"Area of Observation",7]
[null,"Critical_item","L",null,"Deficiency Cause",8]
[null,"Deficiency Type","M",null,"VIQ Ref Number",9]
[null,"Deficiency Cause","N",null,"Risk Value of Obs",10]
[null,"Inspection Type","O",null,"PSC Ref Number",11]
[null,"Equipments","P",null,"PSC MOU ID",12]
[null,"VIQ Reference Number","Q",null,"Action Taken or Required",13]
[null,"Risk Value of the observation","R",null,"Target Date",14]
[null,"PSC Reference Number","S",null,"PO Ref No.",15]
[null,"PSC MOU","T",null,"Status Code",16]
[null,"Observer Code","U",null,"Date Completed",17]
[null,"Target Date","V",null,"Drydock",18]
[null,"Status Code","W",null,"Info Sharing",19]
[null,"Description of Deficiency","X",null,"Critical Item Flag",20]
[null,"Action taken / required","Y",null,"Audit Type",21]
[null,"PO ref no","Z"]
[null,"Date completed","AA"]

{"sheet":"Ship_information","index":19,"n_rows":2,"n_cols":3,"rows_kept":2,"cut":false,"hidden":true,"merged":[]}
["Ship_ID","Ship_Name","FILE_NAME"]
["83","ATHERINA (29-07-2020)","83_1598863843419.xlsm"]

{"sheet":"External_Deficiency_type","index":20,"n_rows":5,"n_cols":3,"rows_kept":5,"cut":false,"hidden":true,"merged":[]}
["TITLE","Type of deficiency_description","ID"]
["Condn of Class / Memo",null,5]
["Defect",null,1]
["Non Conformity",null,2]
["Observation",null,3]

{"sheet":"External_Inspection_type","index":21,"n_rows":11,"n_cols":2,"rows_kept":11,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Cargo Audit",17]
["Flag State Insp.",5]
["ISM Audit",2]
["ISPS Audit",3]
["MLC Audit",1]
["Nav Audit / Verification",8]
["OM Insp. (Eg. SIRE / CDI etc.)",6]
["Others (Eg. Insurance etc.)",12]
["PSC Inspection",4]
["Terminal Insp.",11]

{"sheet":"External_Observer_code","index":22,"n_rows":7,"n_cols":3,"rows_kept":7,"cut":false,"hidden":true,"merged":[]}
["TITLE","Observer_code_description","ID"]
["Class Surveyor",null,4]
["FSC Inspector",null,5]
["Others (Eg. Insurance etc.)",null,9]
["PSC Insp.",null,6]
["SIRE / CDI Insp.",null,8]
["Terminal Insp.",null,7]

{"sheet":"Sheet Version","index":23,"n_rows":2,"n_cols":2,"rows_kept":2,"cut":false,"hidden":true,"merged":[]}
["Version","Title"]
["2.0","Version 2.0"]