{"text_format":"1","workbook":"xlsx","n_sheets":24,"sheets":["Mainsheet","Completed","Calc","Areaofobs","Vessel_type","Deficiency_type","VIQrefno","Equipment_list","PSC_MOU","Inspection_type","Deficiency_Cause","Observer_code","Status_code","PSC_ref_no","Risk_value_of_obs","Year","Month","Date_","Sheet1","Ship_information","External_Deficiency_type","External_Inspection_type","External_Observer_code","Sheet Version"],"not_rendered":{"charts":0,"images":6,"macros":1,"external_links":0,"defined_names":12,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Mainsheet","index":0,"n_rows":17,"n_cols":28,"rows_kept":17,"cut":false,"hidden":false,"merged":[[10,8,10,9],[10,12,10,13],[12,6,12,27],[8,6,8,27]]}
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,"Defect - Damage Monitoring Sheet"]
[]
[null,null,null,null,null,null,null,"Date of Report","24-Dec-2020",null,null,"Ship Name","A MELODY (24-12-2020)"]
[]
[null,null,null,null,null,null,"VERSION : 2.0"]
[]
[]
[]
[null,null,null,null,"ID","UNIQUE ID","Date Recorded","Type of Deficiency","Observer code","Type of Inspection","Description of Deficiency","Equipment Categories","Area of Observation","Deficiency Cause","VIQ Ref Number","Risk Value of Obs","PSC Ref Number","PSC MOU ID","Action Taken or Required","Target Date","PO Ref No.","Status Code","Date Completed","Drydock","Info Sharing","Critical Item","Audit Type","Superintendent Remarks"]

{"sheet":"Completed","index":1,"n_rows":217,"n_cols":28,"rows_kept":217,"cut":false,"hidden":false,"merged":[[10,8,10,9],[10,12,10,13],[12,6,12,27],[8,6,8,27]]}
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,"Defect - Damage Monitoring Sheet"]
[]
[null,null,null,null,null,null,null,"Date of Report","24-Dec-2020",null,null,"Ship Name","A MELODY (24-12-2020)"]
[]
[null,null,null,null,null,null,"VERSION : 2.0"]
[]
[]
[]
[null,null,null,null,"ID","UNIQUE ID","Date Recorded","Type of Deficiency","Observer code","Type of Inspection","Description of Deficiency","Equipment Categories","Area of Observation","Deficiency Cause","VIQ Ref Number","Risk Value of Obs","PSC Ref Number","PSC MOU ID","Action Taken or Required","Target Date","PO Ref No.","Status Code","Date Completed","Drydock","Info Sharing","Critical Item","Audit Type","Superintendent Remarks"]
[null,null,null,null,8218,"84_Wed Nov 06 2019 17:26:45 GMT+0000 (Coordinated Universal Time)","2019-07-01","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Manifold chipping and painting to be carried out","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.41","Medium","","","Derusting and painting of the manifold completed.","2020-02-15","","Completed","2020-01-19","No","No","No","Internal","Noted job in progress. Target date extended."]
[null,null,null,null,8219,"84_Tue Jun 11 2019 17:48:16 GMT+0000 (Coordinated Universal Time)","2019-07-01","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Under Drip tray (Manifold) to be derusted and painted.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.41","Medium","","","Drip tray blasting and painting completed.","2020-01-30","","Completed","2020-01-18","No","No","No","Internal","Noted job in progress."]
[null,null,null,null,9755,"84_15/1/2020 9:00:38 PM","2019-07-01","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Once spares recd. Separator Filter to be installed at the inlet to the dryer. Timer valve with solenoid to be installed at the drain.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Recd and Installed","2019-08-01","","Completed","2019-07-30","Yes","No","No","Internal"]
[null,null,null,null,8220,"84_Tue Jun 11 2019 17:57:28 GMT+0000 (Coordinated Universal Time)","2019-07-01","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Windlass and all winches to be fully blasted and repaint with two coats of primer and one final coat red colour (same as deck) paint.","Deck - Mooring Machinery","Mooring","Equipment Related","9.14","Medium","","","All Windlasses and winches have been blasted and painted","2020-01-31","","Completed","2020-01-19","No","No","No","Internal","Noted maintenance is still in progress."]
[null,null,null,null,9756,"84_16/1/2020 11:13:44 AM","2019-07-01","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Critical spares list to be made and sent to office for approval. Requisitions to be made for missing items.","Documentation","ISM Related","Equipment Related","","","","","List made and sent to office.","2019-07-08","","Completed","2019-07-08","Yes","No","No","Internal"]
[null,null,null,null,8221,"84_Tue Jun 11 2019 18:10:27 GMT+0000 (Coordinated Universal Time)","2019-07-01","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Hydraulic boxes to be blasted from bottom and painted red.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","","","","","Blasting and painting of hydraulic boxes completed.","2020-02-29","","Completed","2020-01-15","No","No","No","Internal","Noted the progress. Target date has been extended."]
[null,null,null,null,9757,"84_16/1/2020 11:15:39 AM","2019-07-01","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Operational spare list to be made with ROBS’s and sent to office for approval","Documentation","ISM Related","Equipment Related","","","","","Made and sent to office","2019-07-08","","Completed","2019-07-08","Yes","No","No","Internal"]
[null,null,null,null,9760,"84_16/1/2020 11:17:44 AM","2019-07-01","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Spares inventory to be taken on a priority and list to be send to the office.","Documentation","ISM Related","Equipment Related","","","","","Completed","2019-08-01","","Completed","2019-09-30","Yes","No","No","Internal"]
[null,null,null,null,9762,"84_14/1/2020 5:18:30 PM","2019-07-01","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Claning of all vent ducts and electrical panels in E/R","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","Vent ducts and electrical panerls cleaned.","2019-07-15","","Completed","2019-07-10","No","No","No","Internal"]
[null,null,null,null,9763,"84_14/1/2020 5:22:40 PM","2019-07-01","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Cleaning and painting of Engine casing and boiler platforms","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","Casing and platforms cleanerd and painted.","2019-08-02","","Completed","2019-07-28","Yes","No","No","Internal"]
[null,null,null,null,9764,"84_14/1/2020 5:25:00 PM","2019-07-01","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","De rusting and painting of ventilation louvers for engine blowers","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","De rusting and painting done","2019-07-16","","Completed","2019-07-20","Yes","No","No","Internal"]
[null,null,null,null,9765,"84_14/1/2020 5:33:53 PM","2019-07-01","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","All missing and damaged steam and fuel oil laggings to be restored/renewed, especially near the ME Cyl lubricator platform- fuel pipes. AE T/C laggings to be renewed with new ones supplied","LSA / FFA","Eng. / Strg. Comp.","Equipment Related","","","","","ER damagaed insulation/laggings replaced with new ones. AE T/C lagging replaced with new ones.","2019-07-03","","Completed","2019-07-31","Yes","No","No","Internal"]
[null,null,null,null,9766,"84_14/1/2020 5:42:26 PM","2019-07-01","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Damaged anti splash tapes to be renewed on high pressure fuel and lub oil lines","LSA / FFA","Eng. / Strg. Comp.","Equipment Related","","","","","All fuel high pressure lines and lubeoil line wrapped with anti splash","2019-07-04","","Completed","2019-07-18","Yes","No","No","Internal"]
[null,null,null,null,9767,"84_15/1/2020 5:10:59 AM","2019-07-01","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","COW line to derusted and painted","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.34","High","","","Spot chipping and painting carried out","2019-07-15","","Completed","2019-07-15","No","No","No","Internal"]
[null,null,null,null,9768,"84_15/1/2020 5:15:45 AM","2019-07-01","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Cargo tankdomes to be derusted and painted","Hull & Tanks","Cargo / Ballast Systems","Equipment Related","8.21","High","","","Derusted and painted","2019-07-10","","Completed","2019-07-10","No","No","No","Internal"]
[null,null,null,null,9769,"84_15/1/2020 5:29:25 AM","2019-07-01","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","LSA/FFA Equipment to be arranged","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","All items well arranged and in place","2019-07-15","","Completed","2019-07-15","No","No","No","Internal"]
[null,null,null,null,9770,"84_15/1/2020 5:35:02 AM","2019-07-01","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Port and Stbd Midship locker to be arranged","Miscellaneous","General Appearance","Equipment Related","","","","","Port and Stbd Midship locker cleaned and arranged","2019-07-15","","Completed","2019-07-15","No","No","No","Internal"]
[null,null,null,null,9771,"84_15/1/2020 5:43:09 AM","2019-07-01","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Manifold driptray supports to be renewed","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","","","","","Manifold driptray supports renewed","2019-07-07","","Completed","2019-07-04","No","No","No","Internal"]
[null,null,null,null,9772,"84_15/1/2020 5:46:57 AM","2019-07-01","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","All supports on deck angle bars to be checked and if required to be welded when vessel is still gas free","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","Equipment Related","","","","","All supports on deck angle bars checked and welded","2019-07-10","","Completed","2019-07-08","No","No","No","Internal"]
[null,null,null,null,9773,"84_15/1/2020 5:53:50 AM","2019-07-01","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Hydraulic line for forepeak ballast tank to be repaired","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","","","","","Hydraulic line for forepeak ballast tank repaired","2019-08-15","","Completed","2019-07-19","No","No","No","Internal"]
[null,null,null,null,9774,"84_15/1/2020 5:58:28 AM","2019-07-01","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Port windlass lever to be capped","Deck - Mooring Machinery","Mooring","Equipment Related","","","","","Port windlass lever capped","2019-07-07","","Completed","2019-07-16","No","No","No","Internal"]
[null,null,null,null,9775,"84_15/1/2020 6:01:12 AM","2019-07-01","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Forward mast railing and platform to be replaced","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","Equipment Related","","","","","Forward mast railing and platform replaced","2019-07-10","","Completed","2019-07-08","No","No","No","Internal"]
[null,null,null,null,9776,"84_15/1/2020 6:05:09 AM","2019-07-01","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Galley - Fridge not working. To be replaced with 3/O cabin fridge","Accommodation","MLC Related","Equipment Related","","","","","New Fridge received at Singapore","2019-07-15","","Completed","2019-07-11","No","No","No","Internal"]
[null,null,null,null,9777,"84_15/1/2020 5:55:31 PM","2019-07-01","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Fire line isolation valves to be overhauled","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","All Fire line isolation valves overhauled","2019-07-30","","Completed","2019-07-12","No","No","No","Internal"]
[null,null,null,null,9778,"84_15/1/2020 6:01:26 PM","2019-07-01","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Foam monitor numbering to be carried out","LSA / FFA","Safety / LSA / FFA","Equipment Related,Inappropriate Procedure","","","","","All foam monitors numbering done","2019-07-15","","Completed","2019-07-04","No","No","No","Internal"]
[null,null,null,null,9779,"84_15/1/2020 6:14:23 PM","2019-07-01","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Mast riser to be cleaned and painted","Cargo Mach.","General Appearance","Equipment Related","8.19","High","","","Mast riser cleaned and painted black","2019-07-20","","Completed","2019-07-03","No","No","No","Internal"]
[null,null,null,null,9780,"84_15/1/2020 6:19:44 PM","2019-07-01","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Repaired conduit line to be painted","Deck - Pipe / Fittings","General Appearance","Equipment Related","","","","","All repaired conduit line painted","2019-07-10","","Completed","2019-07-06","No","No","No","Internal"]
[null,null,null,null,9781,"84_15/1/2020 6:23:32 PM","2019-07-01","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Wrapping on conduit line near 7(P) COT to be removed","Deck - Pipe / Fittings","General Appearance","Equipment Related","","","","","Painted in Yellow","2019-07-15","","Completed","2019-07-06","No","No","No","Internal"]
[null,null,null,null,9782,"84_15/1/2020 6:29:04 PM","2019-07-01","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Laundry housekeeping to be improved","Accommodation,LSA / FFA,Miscellaneous","General Appearance","Behaviour Based,Equipment Related","","","","","All laundries cleaned and posted time of use","2019-07-10","","Completed","2019-07-08","No","No","No","Internal"]
[null,null,null,null,9783,"84_15/1/2020 6:34:34 PM","2019-07-01","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Fireman's outfit to be checked for damage","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.43","High","","","All Fireman's outfit checked for damages and replaced as required","2019-07-07","","Completed","2019-07-04","No","No","No","Internal"]
[null,null,null,null,9784,"84_15/1/2020 6:38:32 PM","2019-07-01","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Cabin and Galley stores to be ordered","Accommodation","MLC Related","External Factors","","","","","Received at SIngapore","2019-07-07","","Completed","2019-07-11","No","No","No","Internal"]
[null,null,null,null,9785,"84_15/1/2020 6:42:16 PM","2019-07-01","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Both accommodation ladder to be painted and to be stencilled with drydock loadtest report date.","Deck - Machinery","General Appearance","Equipment Related","5.47","Medium","","","Both accommodation ladder painted grey and stencilled with drydock loadtest report date.","2019-07-15","","Completed","2019-07-15","No","No","No","Internal"]
[null,null,null,null,9786,"84_15/1/2020 6:54:14 PM","2019-07-01","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","All stencils for last done dates on Deck pipelines and equipment’s to be updated with the latest dates.","Miscellaneous","Cert. & Docu.","Equipment Related","","","","","All stencils for last done dates on Deck pipelines and equipment’s updated with the latest dates.","2019-07-04","","Completed","2019-08-01","No","No","No","Internal"]
[null,null,null,null,9787,"84_15/1/2020 6:08:13 PM","2019-07-01","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Bonding wires on deck to be checked for connectivity and if requird to be renewed","Miscellaneous","Safety / LSA / FFA","Equipment Related","8.48","Medium","","","Bonding wires on deck checked for connectivity and some renewed","2019-07-10","","Completed","2019-07-10","No","No","No","Internal"]
[null,null,null,null,9788,"84_15/1/2020 8:16:16 PM","2019-07-01","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Plugs for IG drain pipe before and after deck seal to be fabricated","Cargo Mach.,Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","","","","","Plugs in place and corroded pipe replaced","2019-07-30","","Completed","2019-08-05","No","No","No","Internal"]
[null,null,null,null,9789,"84_15/1/2020 8:22:17 PM","2019-07-01","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","One aft electrical connection box next to deck workshop to be stencilled with its identification","Accommodation","General Appearance","Equipment Related","","","","","Stencilling carried out","2019-07-15","","Completed","2019-08-11","No","No","No","Internal"]
[null,null,null,null,9790,"84_15/1/2020 11:13:49 PM","2019-07-01","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Fwd. mast light brackets to be replaced","Miscellaneous","Navigation","Equipment Related","","","","","Fabricated new one and placed","2019-07-10","","Completed","2019-08-16","No","No","No","Internal"]
[null,null,null,null,9791,"84_15/1/2020 11:24:54 PM","2019-07-01","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Pumproom ventilators to be derusted and painted. The drain holes to be repaired before painting.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","Both Pumproom blowers derusted & full coat paint applied","2019-07-30","","Completed","2019-08-16","No","No","No","Internal"]
[null,null,null,null,9792,"84_15/1/2020 11:28:44 PM","2019-07-01","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Ships name plate on bridge to be repainted","Miscellaneous","General Appearance","Equipment Related","11.2","Medium","","","Ships name plate on bridge repainted and stencilled","2019-08-30","","Completed","2019-08-25","No","No","No","Internal"]
[null,null,null,null,9793,"84_15/1/2020 11:36:28 PM","2019-07-01","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Hydraulic pipes connecting the hydraulic motors on mooring winches are to be wire brushed and painted ","Deck - Pipe / Fittings","Mooring","Equipment Related","","","","","Wire brushed and painted","2019-07-30","","Completed","2019-08-22","No","No","No","Internal"]
[null,null,null,null,9794,"84_15/1/2020 11:38:47 PM","2019-07-01","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Main mast light base to be painted","Deck - Pipe / Fittings","Navigation","Equipment Related","","","","","Derusted and painted","2019-08-15","","Completed","2019-08-30","No","No","No","Internal"]
[null,null,null,null,9795,"84_15/1/2020 11:40:39 PM","2019-07-01","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Monorail to be derusted and painted","Deck - Pipe / Fittings","General Appearance","Equipment Related","","","","","Derusted and painted","2019-08-30","","Completed","2019-08-30","No","No","No","Internal"]
[null,null,null,null,9796,"84_15/1/2020 11:43:06 PM","2019-07-01","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Garbage compactor to be made operational","Elect. Mach. & Equip.","MARPOL Related","Equipment Related","","","","","Compactor made operational by overhauling the control valve and limit switches. Working satisfactory","2019-08-30","","Completed","2019-08-26","No","No","No","Internal"]
[null,null,null,null,9797,"84_15/1/2020 11:45:15 PM","2019-07-01","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Around the accommodation light brackets to be derusted and painted","Accommodation","General Appearance","Equipment Related","","","","","Derusted and painted","2019-07-15","","Completed","2019-09-14","No","No","No","Internal"]
[null,null,null,null,9798,"84_15/1/2020 11:47:25 PM","2019-07-01","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Hose handling crane to be derusted and painted","Cargo Mach.,Deck - Machinery","Cargo / Ballast Systems","Equipment Related","8.63","High","","","Derusted and painted","2019-10-03","","Completed","2019-10-02","No","No","No","Internal"]
[null,null,null,null,9799,"84_15/1/2020 11:49:29 PM","2019-07-01","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Steam manifolds to be derusted and painted","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","11.4","Very High","","","Derusted and painted","2019-10-10","","Completed","2019-10-05","No","No","No","Internal"]
[null,null,null,null,9800,"84_16/1/2020 5:19:52 AM","2019-07-01","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Old damaged posters including the Luminous signs in engine room, accommodation and deck to be renewed with the ones supplied at the time of takeover.","LSA / FFA","Safety / LSA / FFA","Inappropriate Procedure","","","","","Replaced with new posters","2019-07-07","","Completed","2019-07-06","No","No","No","Internal"]
[null,null,null,null,9803,"84_15/1/2020 8:56:37 PM","2019-07-01","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Control Air dryer membrane to clean and put back","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Membrane renewed","2019-07-07","","Completed","2019-07-15","Yes","No","No","Internal"]
[null,null,null,null,9804,"84_15/1/2020 9:05:53 PM","2019-07-01","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","5TH Engineer has identified all the defective temperature and pressure gauges in the engine room. These are all to be renewed on a priority. ","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","Pressure gauges and temperature gauges renewd","2019-07-08","","Completed","2019-07-31","Yes","No","No","Internal"]
[null,null,null,null,9805,"84_15/1/2020 9:09:04 PM","2019-07-01","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","New filters to be installed on all alternators, turbocharger air intakes and open motors.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Filters renewed","2020-07-06","","Completed","2019-07-17","Yes","No","No","Internal"]
[null,null,null,null,9806,"84_15/1/2020 9:13:16 PM","2019-07-01","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Floats for high level alarm to be installed on port and stbd side bilge wells in steering gear room.","LSA / FFA","Eng. / Strg. Comp.","Equipment Related","","","","","Float installed for STBD bilge well","2019-08-03","","Completed","2019-08-03","Yes","No","No","Internal"]
[null,null,null,null,9807,"84_15/1/2020 9:18:36 PM","2019-07-01","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Emergency Fire pump room bilge high level float not working and same to be replaced","LSA / FFA","Eng. / Strg. Comp.","Equipment Related","","","","","Float replaced","2019-07-03","","Completed","2019-07-09","Yes","No","No","Internal"]
[null,null,null,null,9808,"84_16/1/2020 8:50:30 PM","2019-07-01","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","All spares/boxes/pipes around the funnel deck and on B deck to be cleared and to stowed at secure place.","Miscellaneous","General Appearance","Equipment Related","","","","","Shifted to steering platform","2019-09-30","","Completed","2019-09-23","No","No","No","Internal"]
[null,null,null,null,9809,"84_16/1/2020 11:09:34 AM","2019-07-01","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","MGPS Anodes to be inspected and renewed accordingly","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Anodes inspected","2019-07-18","","Completed","2019-07-27","Yes","No","No","Internal"]
[null,null,null,null,9810,"84_16/1/2020 11:05:53 AM","2019-07-01","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Main Engine and AE Performance to be taken after departure from the yard","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","Performance recorded","2019-07-08","","Completed","2019-07-15","Yes","No","No","Internal"]
[null,null,null,null,9811,"84_16/1/2020 11:23:43 AM","2019-07-01","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Precision instruments are lying haphazardly in the engine store. All instruments to be collected and list made. All instruments to be kept in a separate locker and list to be included in C/E and ETO handover documents.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","Precision instruments arranged in ECR list compiled","2019-07-08","","Completed","2019-07-15","Yes","No","No","Internal"]
[null,null,null,null,9812,"84_16/1/2020 11:27:42 AM","2019-07-01","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Sewage treatment plant pump start/stop float switch is not working. Requisition to be made for the same.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","FLoat switch recived, installed","2019-07-16","","Completed","2019-10-03","Yes","No","No","Internal"]
[null,null,null,null,9813,"84_16/1/2020 11:38:22 AM","2019-07-01","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","To order boiler water test kit from unitor ","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","testing kit reecived","2019-07-14","","Completed","2019-07-12","Yes","No","No","Internal"]
[null,null,null,null,9814,"84_16/1/2020 11:44:44 AM","2019-07-01","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Vessel to order testing chemicals for on-board lub oil test kit.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Onboard testing kit ordere, recived","2019-07-12","","Completed","2019-07-12","Yes","No","No","Internal"]
[null,null,null,null,9815,"84_16/1/2020 2:42:31 PM","2019-07-01","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Calibration of pressure and temp calibrator to be carried out at Singapore.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Pressure and temperature caliberator shore caliberation done.","2019-08-02","","Completed","2019-11-09","Yes","No","No","Internal"]
[null,null,null,null,9816,"84_16/1/2020 2:46:26 PM","2019-07-01","Observation","Owner / Marine / Tech. Suptd.","Ship Staff Insp.","Vessel does not have sufficient spares for overhaul of HFO purifiers. Same to be ordered","E/R - Purifier","Eng. / Strg. Comp.","Equipment Related","","","","","Spares ordered, received at singapore","2019-07-16","","Completed","2019-11-05","Yes","No","No","Internal"]
[null,null,null,null,9817,"84_16/1/2020 2:50:15 PM","2019-07-01","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Ship specific machinery operating procedures to be made and same to be posted near the respective machinery.","Documentation","Eng. / Strg. Comp.","Equipment Related","","","","","operating procedures updated and posted","2019-07-11","","Completed","2019-07-10","Yes","No","No","Internal"]
[null,null,null,null,9818,"84_16/1/2020 2:53:10 PM","2019-07-01","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Engine Room Bilges to be high pressure washed, cleaned and painted. ","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","Bilges cleaned, high pressure","2019-07-16","","Completed","2019-08-17","Yes","No","No","Internal"]
[null,null,null,null,9819,"84_16/1/2020 3:04:54 PM","2019-07-01","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Oxygen and Acetylene Room flame arrestors to be renewed as required by VIQ as these are old.","LSA / FFA","Eng. / Strg. Comp.","Equipment Related","","","","","flame arrestors renewed","2019-07-16","","Completed","2019-07-12","Yes","No","No","Internal"]
[null,null,null,null,9820,"84_16/1/2020 3:06:48 PM","2019-07-01","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Calibration gas for IG O2 Analyser to be ordered.","Inert Gas","Eng. / Strg. Comp.","Equipment Related","","","","","Caliberation gas ordered and received","2019-07-16","","Completed","2020-07-15","Yes","No","No","Internal"]
[null,null,null,null,9821,"84_16/1/2020 3:08:22 PM","2019-07-01","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","IG Scrubber outlet line insulation to remove, leakage to be identified and repaired.","Inert Gas","Eng. / Strg. Comp.","Equipment Related","","","","","Scrubber outlet leak rectified","2019-07-15","","Completed","2019-08-08","Yes","No","No","Internal"]
[null,null,null,null,9822,"84_16/1/2020 3:11:09 PM","2019-07-01","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Insulation near the strng gear entrance from poop deck is damaged and to be repaired","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","Insulation repaired","2019-07-29","","Completed","2019-07-29","Yes","No","No","Internal"]
[null,null,null,null,5352,"84_23/10/2019 3:12:03 PM","2019-07-15","Defect","Ship Staff","Ship Staff Insp.","No1 AUX SEA WATER PUMP MECHANICAL SEAL LEAKING.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.2","Low","","","NO 1 AUX SEA WATER PUMP MECHANICAL SEAL REPLACED WITH NEW SPARE.","2019-07-25","","Completed","2019-07-16","No","No","No","Internal"]
[null,null,null,null,5353,"84_23/10/2019 4:28:31 PM","2019-07-16","Defect","Ship Staff","Ship Staff Insp.","DRINKING WATER PUMP & MOTOR HAVING ABNORMAL NOISE DURING RUNNING.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","",""," DRINKING WATER PUMP AND MOTOR OVERHAULED.","2019-08-10","","Completed","2019-07-23","No","No","No","Internal"]
[null,null,null,null,5354,"84_23/10/2019 4:37:38 PM","2019-08-02","Defect","Ship Staff","Ship Staff Insp.","BOILER GAUGE GLASS FOUND OPAQUE , WATER LEVEL NOT CLEAR.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","8.8","Medium","","","BOILER GAUGE GLASS OVERHAULED.","2019-08-15","","Completed","2019-08-11","No","No","No","Internal"]
[null,null,null,null,5355,"84_23/10/2019 4:43:06 PM","2019-08-04","Defect","Ship Staff","Ship Staff Insp.","NO-2 BOILER WATER CIRCULATING PUMP BADLY LEAKING FROM SHAFT SEAL.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.2","Low","","","NO -2 BOILER WATER CIRCULATING PUMP SHAFT SEAL RENEWED.","2019-08-15","","Completed","2019-08-08","No","No","No","Internal"]
[null,null,null,null,5356,"84_23/10/2019 4:49:21 PM","2019-08-13","Defect","Ship Staff","Ship Staff Insp.","AC COOLING SEA WATER PIPE FOUND SEEPAGE NEAR FLANGE AREA.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","11.4","Very High","","","NEW PIPE FABRICATED AND FITTED IN PLACE.","2019-08-20","","Completed","2019-08-18","No","No","No","Internal"]
[null,null,null,null,9801,"84_16/1/2020 5:23:41 AM","2019-08-28","Observation","Ship Staff","Ship Staff Insp.","Radar and radar tracked target information not connected to ECDIS","Navigation - ECDIS","Navigation","Equipment Related","","","","","Technician visited Singapore anchorage on 05th nov 19, MARTEK ECDIS do not have Radar overlay facility.","2020-02-20","","Completed","2019-11-05","No","No","No","Internal"]
[null,null,null,null,5341,"84_23/10/2019 4:55:02 PM","2019-09-01","Defect","Ship Staff","Ship Staff Insp.","NO1 & 2 FO BURNING PUMP LEAKING FROM MECHANICAL SEAL.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.2","Low","","","Mechanical seal overhauled lapped and assembled. no leaks observed","2019-10-30","AMEL 190017","Completed","2019-11-03","No","No","No","Internal","RO#AMEL190017 - Under processing stage."]
[null,null,null,null,5342,"84_23/10/2019 5:03:19 PM","2019-09-17","Defect","Ship Staff","Ship Staff Insp.","EXHAUST GAS LEAKING FROM BOTTOM CASING OF EGB , SMALL GAS SMELL AT UPPER DECK ACCOMODATION (PORT) AREA.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","EXHAUST GAS BOTTOM EXCESS DOOR BOTTOM BASE PLATE RENEWED AND LEAKAGE RECTIFIED.","2019-11-15","","Completed","2019-10-28","No","No","No","Internal","Did you had any chance to inspect & asscertain nature of leak?"]
[null,null,null,null,5343,"84_23/10/2019 5:07:35 PM","2019-09-20","Defect","Ship Staff","Ship Staff Insp.","ME AIRCOOLER( FWD SIDE)AIR SIDE COVER GASKET LEAKING.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Damaged gasket repaired and leakage rectified.","2019-11-15","AMEL190091","Completed","2019-10-30","No","No","No","Internal","RO#AMEL190091 - Under processing / awaiting quotes."]
[null,null,null,null,5344,"84_23/10/2019 9:28:07 PM","2019-10-01","Defect","Ship Staff","Ship Staff Insp.","SCRUBBER PUMP MECHANICAL SEAL LEAKING.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.2","Low","","","MECHANICAL SEAL CHANGED","2019-11-30","AMEL190081","Completed","2019-11-10","No","No","No","Internal","RO#AMEL190081 is currently under processing."]
[null,null,null,null,5345,"84_23/10/2019 9:34:09 PM","2019-10-01","Defect","Ship Staff","Ship Staff Insp.","NO-2 LUBE OIL PURIFIER INOPERATIVE","E/R - Purifier","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","PURIFIER OVERHAULED.","2019-11-30","AMEL190062","Completed","2019-11-28","No","No","No","Internal","PO#AMEL190062 - Supplied on board at Singapore on 09/11/2019.  Overhaul of Purifier should have commenced by now."]
[null,null,null,null,5346,"84_23/10/2019 9:40:53 PM","2019-10-05","Defect","Ship Staff","Ship Staff Insp.","RUDDER CARRIER GLAND PACKING LEAK","Critical Equip.","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Gland was found not tight properly .Tightened no leaks observed","2020-02-20","AMEL190090","Completed","2019-12-27","No","No","No","Internal","RO#AMEL190090 is currently under processing. Pls re-issue new RO for year 2020 and cancel previous one."]
[null,null,null,null,5347,"84_23/10/2019 9:44:32 PM","2019-10-10","Defect","Ship Staff","Ship Staff Insp.","FREQUENT TUBE LEAKS FOR BOTH MAIN AIR COMPRESSOR.","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","NEW COMPRESSOR FITTED.","2019-11-30","AMEL190053","Completed","2019-11-16","No","No","No","Internal","RO#AMEL190053 is in the processing stage."]
[null,null,null,null,5348,"84_23/10/2019 9:51:49 PM","2019-10-11","Defect","Ship Staff","Ship Staff Insp.","BOILER BOTTOM HOLE PLUG FOUND LEAKING AT HIGH PRESSURE.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Plugs tightned. no leaks at high pressure. Boiler pressed upto 16bar, drain plugs monitiored no leaks.","2019-12-30","","Completed","2019-12-22","No","No","No","Internal","The job is already overdue. Pls advice when you plan to carry out \nsame, otherwise amend the target to a later date."]
[null,null,null,null,5351,"84_23/10/2019 10:19:45 PM","2019-10-16","Defect","Ship Staff","Ship Staff Insp.","MAIN ENGINE EXHAUST TRUNKING INTERMEDIATE BELLOW IN HORIZONTAL POSITION  BETWEEN EGB AND MAIN ENGINE T/C LEAKING.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Compensator found damaged. replaced with sapre compensator.","2019-11-30","","Completed","2019-11-09","No","No","No","Internal","When is the vessel expected to be at anchorage?  What is the current status of the leak?"]
[null,null,null,null,8200,"84_26/11/2019 2:25:35 PM","2019-10-29","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Radar mast to be derusted and painted","Miscellaneous","Structural Condn. / WT integrity ","Equipment Related","","","","","Completed derusting and painting","2020-02-15","","Completed","2020-03-10","No","No","No","Internal",""]
[null,null,null,null,8203,"84_Fri Apr 12 2019 03:35:09 GMT+0000 (Coordinated Universal Time)","2019-11-01","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","No documentation was available on board to establish that both L/Bs on load release hooks were in compliance with MSC.1/Circ.1392. The window to establish compliance ended 31st July 2019.","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.28","Very High","","","Lifeboat release hooks are in compliance with MSC.1/Circ.1392\n\nModification to the lifeboat release and retrieval system carried out in Oct 2011 under previous management.\n\nDocumentation for same is available onboard","2020-01-27","","Completed","2019-12-04","No","No","No","Internal"]
[null,null,null,null,8211,"84_15/12/2019 10:11:09 PM","2019-11-01","Non Conformity","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Temperature and pressure gauges templates has not been uploaded in PAL","Documentation","Eng. / Strg. Comp.","Inappropriate Procedure","10.12","Very High","","","Job updated in Nov month end forms","2020-01-27","","Completed","2019-11-30","No","No","No","Internal"]
[null,null,null,null,8212,"84_15/12/2019 10:13:29 PM","2019-11-01","Non Conformity","Owner / Marine / Tech. Suptd.","Suptd. Insp.","STP air supply found shut off. The blower is abnormal and line connected with service air system. However, this connection too found shut","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.1","Medium","","","Air line valve kept open. notice placed for Do NOT SHUT","2020-01-27","","Completed","2019-11-10","No","No","No","Internal"]
[null,null,null,null,8213,"84_15/12/2019 10:16:20 PM","2019-11-01","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Found a hammer in E/R workshop with metal handle welded to the head.\t\t","Miscellaneous","ISM Related","Human Error","10.1","Medium","","","Metalic handle hammers removed. Notice placed","2020-01-27","","Completed","2019-11-20","No","No","No","Internal"]
[null,null,null,null,8214,"84_16/12/2019 4:23:19 AM","2019-11-01","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Calibration gas certificate for IG O2 analyzer not available on board.","Documentation","Eng. / Strg. Comp.","Industry Issue","","","","","New cylinder received with certificate put in use.Notice placed.","2020-01-27","","Completed","2020-11-20","No","No","No","Internal"]
[null,null,null,null,8215,"84_16/12/2019 4:29:28 AM","2019-11-01","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","EGE pressure drop manometer found without water","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.1","Medium","","","manometer filled with water.Notice placed","2020-01-27","","Completed","2019-11-20","No","No","No","Internal"]
[null,null,null,null,8217,"84_16/12/2019 4:50:20 AM","2019-11-01","Non Conformity","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Enclosed space entries made to #1 HFO Serv Tk and FO Overflow Tk on 16/10/19 & 02/10/19 respectively. It was established that MSDS of","Hull & Tanks","ISM Related","Inappropriate Procedure","5.16","Very High","","","Company Procedure to be followed","2020-01-27","","Completed","2019-12-31","No","No","No","Internal","We suggest that you review same and elaborate on what action is required. We fail to understand the issue regarding this defect."]
[null,null,null,null,8229,"84_Fri Apr 12 2019 03:40:54 GMT+0000 (Coordinated Universal Time)","2019-11-01","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","LOTO Box not available on board.","Miscellaneous","ISM Related","Inappropriate Procedure","","","","","Lock out tag out tags received at Linggi on 19 Feb 2020","2020-02-22","AMEL200009","Completed","2020-02-19","No","No","No","Internal","Will arrange at next storing"]
[null,null,null,null,null,"84_16/12/2019 4:47:23 AM","2019-11-01","Non Conformity","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Different types of cable glands have been used in the pump room explosion proof lights. Same to be verified by ETO so that the validity of the explosion proof lights is maintained.","Elect. Mach. & Equip.","Cargo / Ballast Systems","Equipment Related",null,null,"Not Applicable","Not Applicable","Cable glands checked and verified integrity and its explosion proof validity.","2020-02-27",null,"Completed","2020-12-20","No",null,null,"Internal"]
[null,null,null,null,8202,"84_Fri Apr 12 2019 03:30:29 GMT+0000 (Coordinated Universal Time)","2019-11-05","Defect","FSC Inspector","Flag State Insp.","P & S Lifeboat Hook release mechanism moving parts painted - Observed by Flag state Inspector","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.28","Very High","","","The paint on the moving parts of lifeboat hook release mechanism was immediately removed, followed by buffing. Thin layer of grease was applied over the moving part of hook to prevent from corrosion.                                                      Cautionary note marked near the hooks.\n\n\"DO NOT PAINT HOOKS\"  on both lifeboats","2020-01-30","","Completed","2019-11-13","No","No","No","External"]
[null,null,null,null,8199,"84_26/11/2019 2:16:13 PM","2019-11-06","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Hydraulic/Fresh water/ Airline corroded/wasted on Main deck forward. Same to be renewed.","Deck - Pipe / Fittings","General Appearance","Equipment Related","","","","","Corroded FW/Airline on main deck renewed with new pipes onboard. ","2020-01-06","","Completed","2019-11-30","No","No","No","Internal"]
[null,null,null,null,9752,"84_16/1/2020 5:39:54 AM","2019-11-06","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","IG line U-bolts and stood bolts need to be maintained/painted, maybe several needs to be replaced  located in front of pump room)","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","Equipment Related","","","","","IG Line stood bolts for IG lime isolation valve replaced, renewing of IG line U Bolts Completed","2020-02-28","","Completed","2020-02-10","No","No","No","Internal","Target date revised. Job in progress."]
[null,null,null,null,9802,"84_16/1/2020 5:34:17 AM","2019-11-06","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Pump room Exh. Fans Flame arrestor the squares NOT proper dimension (big ), to be replaced\n\n\n\n","LSA / FFA,Miscellaneous","Cargo / Ballast Systems","Equipment Related","","","","","Fine Mesh flame screen inserted below pumproom exhaust blower frames.","2019-12-06","","Completed","2019-11-10","No","No","No","Internal"]
[null,null,null,null,9823,"84_16/1/2020 3:16:06 PM","2019-11-06","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","F.O SETT. TNK to M/E the Twin filter found leaking, to be rectified","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Filter leak rectified, cleaned, painted","2019-12-08","","Completed","2019-12-05","No","No","No","Internal"]
[null,null,null,null,9824,"84_16/1/2020 3:19:19 PM","2019-11-06","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Steering gear motors found dirty, to be cleaned and painted, PS hydraulic block the pressure gauge found leaking, to be rectified.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","Motors cleaned, hydraulic block cleaned, pressure gauge leak rectified","2019-11-30","","Completed","2019-11-25","No","No","No","Internal"]
[null,null,null,null,9825,"84_16/1/2020 3:21:22 PM","2019-11-06","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","F.O No1 STBD TNK the quick closing valve found leaking, to be rectified ","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","leak rectified, Valve cleaned painted","2019-12-04","","Completed","2019-11-20","No","No","No","Internal"]
[null,null,null,null,9826,"84_16/1/2020 3:33:09 PM","2019-11-06","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Engine room Lower Platform all Pumps found without axle guard protection, wire mesh Guards to be installment","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","axle guard protection installed.","2019-11-21","","Completed","2019-11-14","No","No","No","Internal"]
[null,null,null,null,9827,"84_16/1/2020 3:37:26 PM","2019-11-06","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","L.O SETTL TNK from steam pipe missing valves’ hand wheel","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","hand wheel installed","2019-11-21","","Completed","2019-11-10","No","No","No","Internal"]
[null,null,null,null,9828,"84_16/1/2020 3:49:10 PM","2019-11-06","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Fan rooms Louvers found rusted/wasted ","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Rusted louvers fabricated","2019-12-30","","Completed","2019-11-26","No","No","No","Internal"]
[null,null,null,null,null,"84_16/1/2020 5:44:59 AM","2019-11-06","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Deck from manifolds IWO to FWD found spot rusted (COT’s domes/manholes, WBT ’manholes/ve nts ) to be maintained and painted","Deck - Pipe / Fittings","General Appearance","Equipment Related,External Factors",11.1,"High","Not Applicable","Not Applicable","Main deck completed from midship to fwd. Railings and catwalk completed.","2020-05-25",null,"Completed","2020-12-14","No",null,null,"Internal"]
[null,null,null,null,null,"84_16/1/2020 5:42:22 AM","2019-11-06","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Accommodation superstructures& Funnel casing found spot rusted. To be maintained and painted","Accommodation","General Appearance","Equipment Related,External Factors",null,null,"Not Applicable","Not Applicable","Funnel casing derusting completed,Accomodation block front section de-rusting and painting completed. Aft accommodation block de-rusting and painting completed","2021-01-31",null,"Completed","2021-01-02","No",null,null,"Internal"]
[null,null,null,null,8198,"84_26/11/2019 2:05:26 PM","2019-11-10","Breakdown","Ship Staff","Ship Staff Insp.","Stbd. pumproom damper operating valve found ceased. Crack found in body and damper not closing completely.","Critical Equip.","Emgcy. Systems","Equipment Related","5.19","Medium","","","Damper operating valve removed from location and hot work carried out in E/rm workshop. Shaft well lubricated.","2019-11-30","","Completed","2019-11-20","No","No","No","Internal"]
[null,null,null,null,8224,"84_14/11/2019 10:07:33 AM","2019-11-11","Defect","Ship Staff","Ship Staff Insp.","Economiser bottom side plate holed.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.19","Very High","","","Plates welded on to bottom and side casing from inside.","2019-12-24","","Completed","2019-12-24","No","No","No","Internal"]
[null,null,null,null,8201,"84_25/11/2019 6:21:55 PM","2019-11-12","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","#1 E/R Blower some of fan louvers found wasted","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","16 nos of plates replaced with new spare","2019-11-30","","Completed","2019-11-26","No","No","No","External"]
[null,null,null,null,8204,"84_Fri Apr 12 2019 03:58:41 GMT+0000 (Coordinated Universal Time)","2019-11-18","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","12.20.05.011.03 - Pre Arrival and Commencement of Cargo Operation Checklist - 05 Sept 2019 filled incorrectly :\n\na) Sec C Pt. 32 - Butterworth Heater Valves: marked as NA whereas Vessel fitted with Tank Cleaning Heater.\n\nb) Sec E Pt 3 - Shut Status of Manually Operated Valves Checked (These are all manual valves on Deck/Pump Room) - Marked as NA.\n\nc) Checklist marked completed on 05 Sept 2300 Hrs. However, Vessel lined up and double checked by D/Off (Sec C - Pt.24) at 2312 Hrs as mentioned in CCR Log. Also, hose connection not completed till 2300 Hrs - Ref Pt 4 Sec C of Pre Arrival Checklist (Version 3) \n\n","Miscellaneous","Cargo / Ballast Systems","Inappropriate Procedure","8.1","Very High","","","Corrective action: Checklist reviewed, corrected and initials made.                                                             Preventive action: Due care to be exercised when filling up a checklist. Once the checklist is filled up, same to be verified by Duty Officer on watch and a log entry to be made. Any short comings to be brought to the notice of chief officer. In short, a cross audit of checklist to be carried out on spot by another officer to avoid one-man error. Briefing of all Deck officers carried out. ","2019-12-10","","Completed","2019-12-01","No","No","No","Internal"]
[null,null,null,null,8205,"84_Fri Apr 12 2019 04:01:52 GMT+0000 (Coordinated Universal Time)","2019-11-18","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","CCR Movement Log – 02 Nov 2019 for discharge operation at Linggi – No entry for Starting of IG sighted prior commencement of discharging.","Miscellaneous","Cargo / Ballast Systems","Inappropriate Procedure","8.1","Very High","","","Corrective action: Missing entry inserted for starting of IG in CCR Log for 02 Nov 19 for operation at Linggi - Entry obtained from IG recorder.                                                                        Preventive action: Entries in CCR movement log will be made as per GSM procedures 12.21.06.001.01 . Briefing of all deck officers Carried out.","2019-12-10","","Completed","2019-12-01","No","No","No","Internal"]
[null,null,null,null,8206,"84_Fri Apr 12 2019 04:03:43 GMT+0000 (Coordinated Universal Time)","2019-11-18","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","12.20.05.011.04 - Pre Arrival and Commencement of Cargo Operation Checklist - Discharging completed on 02 Nov 2019\n\nSec D Pt 15 - Has visual check of ballast surface in WBT been carried out prior de-ballasting is marked as YES during Discharge Operations. However all ballast tanks adjacent to cargo spaces recorded as Nil sounding in Hourly Discharge Log.\n\n","Miscellaneous","Cargo / Ballast Systems","Inappropriate Procedure","8.1","Very High","","","Corrective action: Checklist reviewed, corrected and initials made.                                                                 Preventive action: Due care to be exercised when filling up a checklist. Once the checklist is filled up, same to be verified by Duty Officer on watch and a log entry to be made. Any short comings to be brought to the notice of chief officer. In short, a cross audit of checklist to be carried out on spot by another officer to avoid one-man error. Briefing of all deck officers carried out.","2019-12-10","","Completed","2019-12-01","No","No","No","Internal"]
[null,null,null,null,8207,"84_Fri Apr 12 2019 04:05:29 GMT+0000 (Coordinated Universal Time)","2019-11-18","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Entries in CCR movement book not made as per GSM procedures 12.21.06.001.01. \n\nEvidence for independent check - Line up for venting not sighted. \n\nEvidence of Tests and Checks Prior cargo operations not sighted. \n\n","Miscellaneous","Cargo / Ballast Systems","Inappropriate Procedure","8.1","Very High","","","Corrective action: All Officers briefed about the shortcoming and advised to make entry in CCR log as per GSM procedure 12.21.06.001.01.                           Preventive action: Entries in CCR movement log will be made as per GSM procedures 12.21.06.001.01 with due vigilance.\n\nLaminated copy of same posted in CCR.\n\n","2019-12-01","","Completed","2019-12-01","No","No","No","Internal"]
[null,null,null,null,8208,"84_Fri Jul 12 2019 12:33:03 GMT+0000 (Coordinated Universal Time)","2019-11-18","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Bunker Transfer Plan / Checklist 12.04.08.011.01 Section 7 - Monitoring of H2S/Benzene Vapors: \n\nBenzene reading measured by detector tubes shall be mentioned < Min value that can be measured by the specific tube. For example, by Gastec tubes Min measurable value is 0.05 ppm, hence in that case benzene shall be mention <0.05 ppm (if no discoloration observed)\n\nUnderstand vessel has kept the Gas tubes as evidence of monitoring\n\n","Documentation","Cert. & Docu.","Inappropriate Procedure","","","","","Checklist reviewed and corrections made. From now onwards if no discoloration observed in checklist <0.05ppm will mention. All Engineers briefed about mentioning gas check values.","2019-11-29","","Completed","2019-12-02","No","No","No","Internal"]
[null,null,null,null,8209,"84_Fri Jul 12 2019 12:37:05 GMT+0000 (Coordinated Universal Time)","2019-11-18","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","12.04.08.011.00 - Bunker Safety Checklist: \n\nBunker Safety Checklist to be signed by Chief Officer after completion of the Checklist done by Chief Engineer. \n\nHowever, Chief Off Signed the checklist at 2040 Hrs and Checklist completed by Chief Engineer - 2050 Hrs.\n\n","Documentation","Cert. & Docu.","Inappropriate Procedure","","","","","Checklist reviewed and corrections made. All Engineers briefed about importance of filling checklists and timings should be appropriate as required. ","2019-11-29","","Completed","2019-12-02","No","No","No","Internal"]
[null,null,null,null,8210,"84_Fri Jul 12 2019 12:43:40 GMT+0000 (Coordinated Universal Time)","2019-12-03","Defect","Ship Staff","Ship Staff Insp.","JCW preheater 30%  tubes are  plugged  and frequintely leaking","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","All pipes were renewed with new ones by ER staff","2019-12-12","","Completed","2019-12-12","No","No","No","Internal"]
[null,null,null,null,8230,"84_15/12/2019 3:01:41 PM","2019-12-12","Defect","Ship Staff","Ship Staff Insp.","#1 MAC unloader leaking","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Spare unloader O ring fabricated and assembled.","2020-02-03","","Completed","2020-01-18","No","No","No","Internal","Pls raise RO# for the required spare, if not already done."]
[null,null,null,null,9761,"84_8/1/2020 4:19:16 PM","2019-12-28","Observation","Ship Staff","Ship Staff Insp.","Cooling sea water thre way valve to oveboard jammed, unable to rotate.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Valve removed, cleaned assembeld, working satisfactory","2020-01-07","","Completed","2020-01-05","No","No","No","Internal"]
[null,null,null,null,9748,"84_8/1/2020 4:15:13 PM","2020-01-06","Observation","Ship Staff","Ship Staff Insp.","Oil seal Leaking","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Inner bush removed and turned 180degree, assembled, same oil seal used. compressor in operational","2020-02-28","AMEL 200012","Completed","2020-01-20","No","No","No","Internal"]
[null,null,null,null,9749,"84_8/1/2020 4:41:55 PM","2020-01-06","Observation","Ship Staff","Ship Staff Insp.","Selector valve of Port windlass slightly sweating","Deck - Mooring Machinery","Mooring","Equipment Related","","","","","Selector valve replaced with spare used one","2020-02-20","200017","Completed","2020-09-28","No","No","No","Internal","Selector valve O ring to replace to rectify leakage."]
[null,null,null,null,9750,"84_9/1/2020 6:36:35 AM","2020-01-06","Observation","Ship Staff","Ship Staff Insp.","Hose handling crane Slewing operating valve oil sea leaking","Cargo Mach.,Deck - Machinery","Cargo / Ballast Systems","Equipment Related","8.5","Very High","","","Repaired by putting an extra o-ring, teflon tape and some silicone. Made threaded hole arrangement for securing the operating lever.","2020-03-06","200055","Completed","2020-09-08","No","No","No","Internal"]
[null,null,null,null,11720,"84_19/2/2020 6:24:28 AM","2020-01-20","Observation","Ship Staff","Ship Staff Insp.","Scrubber venturi pipe leaking","Inert Gas","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","New pipe fabricated and installed, all flexible pipes replaced with new.                                                 JO number V-AMEL004481/20","2020-02-15","","Completed","2020-02-10","No","No","No","Internal"]
[null,null,null,null,11721,"84_19/2/2020 3:37:31 PM","2020-02-03","Observation","Ship Staff","Ship Staff Insp.","Air vent valve leaking from boiler side","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","Boiler depressurised, gasket renewed","2020-02-20","","Completed","2020-02-19","No","No","No","Internal"]
[null,null,null,null,11722,"84_1/3/2020 9:38:29 AM","2020-02-24","Observation","Ship Staff","Ship Staff Insp.","Reefer compressor #1 not devoloping pressure,found valve plate crack.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Awaiting spare for replacing valve plate","2020-05-10","200077","Completed","2020-04-24","No","No","No","Internal"]
[null,null,null,null,11723,"84_3/3/2020 8:04:45 AM","2020-02-25","Observation","Ship Staff","Ship Staff Insp.","Stbd. windlass hydraulic stainless pipes found leaking","Deck - Mooring Machinery","Mooring","Equipment Related","9.14","Medium","","","Leak rectified","2020-05-25","","Completed","2020-04-25","No","No","No","Internal"]
[null,null,null,null,11724,"84_3/3/2020 8:15:04 AM","2020-02-28","Observation","Ship Staff","Ship Staff Insp.","VRCS main pressure line aft of manifold found leaking close to omega bend","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","","","","","Omega bend cropped, new bend prepared and inserted with Ermato couplings","2020-05-28","","Completed","2020-04-12","No","No","No","Internal"]
[null,null,null,null,11718,"84_12/3/2020 5:00:22 PM","2020-03-12","Defect","Ship Staff","Ship Staff Insp.","Aux. CSW Pump no1 and 2 suction valve not holding. ","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Gear box taken out and readjusted after partly ginding one teeth and adjusted to fully closed position. Both valves found holding good.Maintenance on pump and filter can be performed with ease. ","2020-06-12","AMEL200088","Completed","2020-10-12","No","No","No","Internal"]
[null,null,null,null,11725,"84_18/3/2020 1:03:20 PM","2020-03-12","Observation","Ship Staff","Ship Staff Insp.","Main steam line valve body is corroded and holed in one location","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","","","","","Valve renewed","2020-05-10","","Completed","2020-04-28","No","No","No","Internal"]
[null,null,null,null,11715,"84_18/3/2020 1:50:08 PM","2020-03-14","Defect","Ship Staff","Ship Staff Insp.","On routine inspection it was found that when the dead man alarm was triggered it was displayed as 110v low insulation alarm on AMS.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","NOTICE PUT NEAR THE DEAD MAN ALARM PANEL.","2020-06-06","","Completed","2020-07-15","No","No","No","Internal"]
[null,null,null,null,null,"84_18/3/2020 1:53:22 PM","2020-03-14","Defect","Ship Staff","Ship Staff Insp.","On routine checks of alarm it was found that there was no alarm triggered on AMS for the Hydraulic power pack abnormal. The alarm was only displayed on the local starter panel.","Deck - Mooring Machinery","Eng. / Strg. Comp.","Equipment Related",null,null,"Not Applicable","Not Applicable","HPU sytem trips at high lube oil temperature and low level alarm. Abnormal alarm is not required for AMS.","2020-06-06",null,"Completed","2020-12-20","No",null,null,"Internal"]
[null,null,null,null,11726,"84_1/5/2020 9:02:07 AM","2020-03-16","Observation","Ship Staff","Nav Audit / Verification","Deck Officer unaccompanied during SCBA air bottle recharging","Miscellaneous","ISM Related","Inappropriate Procedure","","","","","It was brought to the notice of all engineers that one of them should be present during operation of SCBA compressors during charging of air bottles.To be confirmed by senior management that deck officer and engineer are present during operation of SCBA compressor for charging of air bottles ","2020-06-16","","Completed","2020-04-22","No","No","No","Internal"]
[null,null,null,null,11714,"84_18/3/2020 1:39:16 PM","2020-03-18","Defect","Ship Staff","Ship Staff Insp.","QUICK CLOSING VALVE FOR DG FUEL SUPPLY ON HFO SERVICE TANK NO.2 DEFECTIVE","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","QUICK CLOSING MECHANISM MADE OPERATIONAL","2020-06-18","AMEL200091","Completed","2020-06-17","No","No","No","Internal"]
[null,null,null,null,11717,"84_18/3/2020 1:28:17 PM","2020-03-18","Defect","Ship Staff","Ship Staff Insp.","Quick closing valve for Cylinder oil tank defective","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","QUICK CLOSING MECHANISM MADE OPERATIONAL","2020-06-18","AMEL200091","Completed","2020-06-17","No","No","No","Internal"]
[null,null,null,null,13090,"84_17/5/2020 8:16:28 AM","2020-04-11","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Main Deck – Area forward of Midship is still pending for Hydro blasting and painting. To be carried out at the earliest","Miscellaneous","General Appearance","Equipment Related","11.3","Medium","","","To be hydroblasted and painted.","2020-07-11","","Completed","2020-08-31","No","No","No","Internal"]
[null,null,null,null,13091,"84_17/5/2020 8:07:35 AM","2020-04-11","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Hose handling Crane- Operating Block is leaking","Cargo Mach.,Deck - Machinery","Cargo / Ballast Systems","Equipment Related","8.5","Very High","","","Repaired by putting an extra o-ring, teflon tape and some silicone. Made threaded hole arrangement for securing the operating lever.","2020-06-11","AMEL200055","Completed","2020-09-08","No","No","No","Internal"]
[null,null,null,null,13096,"84_17/5/2020 8:28:16 AM","2020-04-11","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","The bridge Wings pillars to be derusted and painted as it is giving a very poor appearance from outside.","Accommodation","General Appearance","Equipment Related","11.8","Low","","","To be de rusted and painted.","2020-07-11","","Completed","2020-08-13","No","No","No","Internal"]
[null,null,null,null,13107,"84_17/5/2020 4:23:01 PM","2020-04-11","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Refer compressor no.1 is not working. To be investigated.","E/R - Pumps,Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Investigate the cause and rectify problem","2020-05-11","","Completed","2020-04-24","No","No","No","Internal"]
[null,null,null,null,13108,"84_17/5/2020 4:11:56 PM","2020-04-11","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Some pipes and foundations in engine room bilgeswere found rusted especially at forward end. Same to be derusted and painted.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","External Factors","10.29","Medium","","","Derusting and painting","2020-06-11","","Completed","2020-05-28","No","No","No","Internal"]
[null,null,null,null,13109,"84_17/5/2020 4:15:29 PM","2020-04-11","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Foundation of pumps in the E/R Bilges are rusty. To be derusted and painted","E/R - Pumps","Emgcy. Systems","Equipment Related","10.29","Medium","","","derusting and painting","2020-07-11","","Completed","2020-05-28","No","No","No","Internal"]
[null,null,null,null,13110,"84_17/5/2020 8:36:17 AM","2020-04-11","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Mid ship stores exterior to be derusted and painted. ","Miscellaneous","General Appearance","Equipment Related","11.12","Low","","","To be de rusted and painted","2020-06-11","","Completed","2020-05-15","No","No","No","Internal"]
[null,null,null,null,13111,"84_17/5/2020 8:31:02 AM","2020-04-11","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Top side near 2 Wb port side paint pealed off due to mechanical damage. Same to be touched up.","Hull & Tanks","General Appearance","Equipment Related","11.3","Medium","","","Touch up to be carried out.","2020-07-11","","Completed","2020-06-01","No","No","No","Internal"]
[null,null,null,null,13112,"84_17/5/2020 8:10:57 AM","2020-04-11","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Crane winch is rusted","Cargo Mach.,Deck - Machinery","Cargo / Ballast Systems","Equipment Related","8.5","Very High","","","De rusted and painted","2020-06-11","","Completed","2020-06-02","No","No","No","Internal"]
[null,null,null,null,13113,"84_17/5/2020 8:23:40 AM","2020-04-11","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Fresh water line on Deck is in poor condition. Corroded sections to be renewed.","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.4","Very High","","","Corroded sections of FW pipes renewed","2020-07-11","","Completed","2020-06-04","No","No","No","Internal"]
[null,null,null,null,13114,"84_17/5/2020 8:46:35 AM","2020-04-11","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","All steam manifolds on deck forward of midship to be derusted and touched up with paint","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","11.4","Very High","","","Steam coils forward of manifold de rusted and painted.","2020-07-11","","Completed","2020-06-24","No","No","No","Internal"]
[null,null,null,null,11727,"84_1/5/2020 8:10:14 AM","2020-04-11","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Fire hose box, located outside accommodation UDK stbd side did not have locking hasp to close the door.","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","Locking hasp renewed","2020-07-11","","Completed","2020-04-15","No","No","No","Internal"]
[null,null,null,null,11728,"84_1/5/2020 8:13:19 AM","2020-04-11","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","The location of following spool pieces not stencilled.\n\n1) Engine room to slop tank\n\n2) IG Line to Cargo line","Miscellaneous","ISM Related","Equipment Related","","","","","Location of spool pieces marked","2020-07-11","","Completed","2020-04-20","No","No","No","Internal"]
[null,null,null,null,11729,"84_1/5/2020 8:16:34 AM","2020-04-11","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","List of security equipment is not maintained as per SSP SEction 08.03.","Miscellaneous","ISPS Related","Equipment Related","","","","","Equipment list maintained as per SSP 08.03","2020-07-11","","Completed","2020-04-20","No","No","No","Internal"]
[null,null,null,null,null,"84_17/5/2020 8:32:52 AM","2020-04-11","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Accommodation from port side next to pumproom has lot of rust stains. Same to be derusted and painted","Accommodation","General Appearance","Equipment Related",11.13,"Low","Not Applicable","Not Applicable","Derusting & Full Coat Painting of Accommodation Front carried out.","2020-07-11",null,"Completed","2020-12-30","No",null,null,"Internal"]
[null,null,null,null,null,"84_17/5/2020 8:37:20 AM","2020-04-11","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Forecastle store is dirty. To be derusted and painted. ","Miscellaneous","General Appearance","Equipment Related",11.12,"Low","Not Applicable","Not Applicable","Forecastle cleaned. Spot chipping and painting carried out. ","2020-06-11",null,"Completed","2020-12-23","No",null,null,"Internal"]
[null,null,null,null,null,"84_17/5/2020 8:48:11 AM","2020-04-11","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","About 50% of the accommodation block is still pending for derusting and painting. To be completed.","Accommodation","General Appearance","Equipment Related",11.8,"Low","Not Applicable","Not Applicable","Accomodation sides and front section de-rusting and painting completed.Aft section completed","2021-01-31",null,"Completed","2021-01-02","No",null,null,"Internal"]
[null,null,null,null,null,"84_17/5/2020 8:19:07 AM","2020-04-11","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Hydraulic lines, cargo pipelines, fire line pipes and supports on deck require de rusting and painting","Deck - Pipe / Fittings","General Appearance","Equipment Related",null,null,"Not Applicable","Not Applicable","De-rusting and painting completed for Hydraulic lines, Cargo pipelines, Fire line pipes and support.","2021-03-31",null,"Completed","2020-12-22","No",null,null,"Internal"]
[null,null,null,null,null,"84_17/5/2020 8:21:11 AM","2020-04-11","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","VRCS pipelines are in poor condition. Corroded sections to be renewed. ","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related",11.4,"Very High","Not Applicable","Not Applicable","Pipe section for VRCS received at Fujairah on 08-Dec-2020.Renewal of pipelines carried out.","2021-04-30",null,"Completed","2021-01-14","No",null,null,"Internal"]
[null,null,null,null,null,"84_17/5/2020 8:25:21 AM","2020-04-11","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Deck airline is in poor condition. Corroded sections to be renewed.","Deck - Pipe / Fittings","General Appearance","Equipment Related",11.4,"Very High","Not Applicable","Not Applicable","Deck airline pipes received in Fujairah on 08-Dec-2020. Renewal of pipelines carried.","2021-01-30",null,"Completed","2021-01-10","No",null,null,"Internal"]
[null,null,null,null,11719,"84_1/5/2020 8:23:31 AM","2020-04-14","Defect","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","Cargo Tank Pressure Monitoring system was independent of the gauging system. All tanks were common and maintained at about 80mb. Error readings of 1072mb, 1233mb, -152mb and 3mb were observed for No.2P, 3P, 5S and 6P cargo tanks respectively.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.13","Medium","","","Zener barrier received and issue rectified.\n\n\n\n","2020-07-14","","Completed","2020-07-10","No","No","No","External"]
[null,null,null,null,11730,"84_1/5/2020 8:28:20 AM","2020-04-14","Observation","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","SPM pick-up line had to be lead around two pedestal fairleads before being fed to the stowage winch. Total aggregate of the angle of change of direction was more than 90 deg.","Deck - Pipe / Fittings","Mooring","Equipment Related","9.26","Low","","","This is design of the vessel from shipyard. Same has been approved by Class. ","2020-07-14","","Completed","2020-04-28","No","No","No","External"]
[null,null,null,null,11731,"84_1/5/2020 8:43:50 AM","2020-04-14","Observation","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","Most recent LO analysis report dated 17 Feb 2020 indicated \"Attention\" for AE#3 , Remote control v/v, Stern tube , M/E filter. \"Urgent for emergency diesel generator\"","Miscellaneous","ISM Related","Inappropriate Procedure","10.7","Medium","","","Bunker sample analysis for HFO Bunker taken on (10 April 2020) received.\n\nEmergency Diesel Generator which had ‘Urgent’ in the last LO analysis, Root cause identified, rectified and taken fresh Oil.\n\nOther machinery AE#3, Remote Control Valve, Stern tube and ME before filters which had attention, corrective action taken as follows.\n\nAE#3 – Sump oil renewal carried out.\n\nRemote Control VV- Partial replenishment of oil carried out.\n\nStern tube- Filling line modified to prevent cross contamination with ME system Oil and renewal of Oil carried out.\n\nME before filters- Both LO purifiers were run at minimum feed and at 95 deg to remove water as per report says  ‘oil content with a small amount of water which is not considered harmful’. Partial replenishment of oil carried out.\n\nEvidence of corrective actions taken was entered in PMS (PAL) and same shown to SIRE inspector.\n\n","2020-07-14","","Completed","2020-04-14","No","No","No","External"]
[null,null,null,null,13115,"84_25/5/2020 11:36:22 AM","2020-05-09","Observation","Owner / Marine / Tech. Suptd.","Cargo Audit","BHC should be 80% of ship design MBL and rendering to be carried out at 60% of ship design MBL ","Deck - Mooring Machinery","Mooring","Equipment Related","9.7","Medium","","","Vessel carried out annual BHC test on 18 Jun 2020. All winches are marked with BHC 63.2T(80% of ship design MBL) and Rendering 47.4T(60% of ship design MBL).","2020-08-09","","Completed","2020-06-18","No","No","No","Internal"]
[null,null,null,null,13116,"84_25/5/2020 11:38:53 AM","2020-05-09","Observation","Owner / Marine / Tech. Suptd.","Cargo Audit","Pre arrival checklist should be filled up seperately for STS operations not conducted consecutively","Miscellaneous","Cert. & Docu.","Inappropriate Procedure","","","","","All officers briefed about the short coming.                            Henceforth separate pre arrival checklist to be filled for separate STS operations.\n\nVessel currently anchored at Singapore OPL, awaiting discharge operation.                               Shortcoming will be complied with in the next STS/Cargo operation and officers briefed about the same.\n\n","2020-08-09","","Completed","2020-06-18","No","No","No","Internal"]
[null,null,null,null,null,"84_22/5/2020 10:38:10 AM","2020-05-22","Observation","Ship Staff","Ship Staff Insp.","Pumproom gas detection system O2 sensor is expired and cannot be calibrated. Vessel raised a PO(AMEL200033) for new O2 sensor but received wrong supply.","Miscellaneous","Cargo / Ballast Systems","Equipment Related",null,null,"Not Applicable","Not Applicable","Sensor replaced with new spare and sytem working satisfactory.","2020-08-22",null,"Completed","2020-12-18","No",null,null,"Internal"]
[null,null,null,null,null,"84_22/5/2020 10:43:49 AM","2020-05-22","Observation","Ship Staff","Ship Staff Insp.","VECS oxygen alarm monitor sensors are expired and same cannot be calibrated.","Miscellaneous","Cargo / Ballast Systems","Equipment Related",8.17,"Low","Not Applicable","Not Applicable","Received new oxygen sensors and replaced.","2021-03-31","AMEL210005","Completed","2021-01-03","No",null,null,"Internal"]
[null,null,null,null,13106,"84_27/5/2020 9:43:15 PM","2020-05-25","Defect","Ship Staff","Ship Staff Insp.","2P BUNKER TANK FILLING VALVE NOT HOLDING; GATE VALVE IN BUNKER LINE TRANSFER SYSTEM ON DECK NOT HOLDING","Deck - Pipe / Fittings","Eng. / Strg. Comp.","Equipment Related","","","","","RENEW VALVES","2020-08-25","AMEL200093","Completed","2020-07-23","No","No","No","Internal"]
[null,null,null,null,13101,"84_30/5/2020 7:19:50 AM","2020-05-26","Defect","Ship Staff","Ship Staff Insp.","2P Fuel oil tank vent pipe on deckis corroded and has got holed.","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","External Factors","","","","","Cold repair carried out on Corroded section","2021-05-25","","Completed","2020-08-10","Yes","No","No","Internal"]
[null,null,null,null,null,"84_1/6/2020 11:14:19 AM","2020-05-26","Defect","Ship Staff","Ship Staff Insp.","Vent heads for Clean Bilge tank , DO Tank (stbd) and Bilge Holding tank are in very poor condition and needs renewal.","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","Equipment Related",null,null,"Not Applicable","Not Applicable","Vent heads for clean bilge tank , DO tank and bilge holding tank renewed with spares received.","2021-01-25",null,"Completed","2021-01-06","No",null,null,"Internal"]
[null,null,null,null,13103,"84_3/6/2020 3:33:33 PM","2020-06-03","Defect","Ship Staff","Ship Staff Insp.","DG 1 GOVERNOR ERRATIC OPERATION","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","RENEW GOVERNOR","2020-09-03","AMEL200155","Completed","2020-07-23","No","No","No","Internal"]
[null,null,null,null,null,"84_24/6/2020 3:38:38 PM","2020-06-03","Observation","Ship Staff","Ship Staff Insp.","Ballast strainers found wasted at some locations.","Miscellaneous","Cargo / Ballast Systems","Equipment Related",null,null,"Not Applicable","Not Applicable","Repairs carried out on wasted section.","2021-01-31",null,"Completed","2021-01-05","No",null,null,"Internal"]
[null,null,null,null,13105,"84_24/6/2020 4:12:24 PM","2020-06-24","Observation","Ship Staff","Suptd. Insp.","Midship draft gauge vent heads are wasted.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","11.7","High","","","Vent heads to be renewed","2020-09-24","AMEL200130","Completed","2020-08-14","No","No","No","Internal"]
[null,null,null,null,13546,"84_16/7/2020 6:18:34 PM","2020-07-09","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","2 bolts on No.3 COP Manifold flange small in size, to replace with new received","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","","","","","Bolts received in singapore on 10 Jul 20 and renewed.","2020-07-14","","Completed","2020-07-11","No","No","No","Internal"]
[null,null,null,null,13547,"84_16/7/2020 6:38:45 PM","2020-07-09","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Stbd side boat deck, natural vents stencil missing as recent maintenance carried out, re stencilling of vents to be carried out.","Deck - Pipe / Fittings","MARPOL Related","Equipment Related","","","","","All vents stencilled.","2020-07-10","","Completed","2020-07-11","No","No","No","Internal"]
[null,null,null,null,13548,"84_16/7/2020 6:53:26 PM","2020-07-09","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Stbd midship locker outside lifebuoy rope became brittle,to replace with new rope,non kink type","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.31","High","","","Lifebuoy grabline renewed.","2020-07-11","","Completed","2020-07-11","No","No","No","Internal"]
[null,null,null,null,13549,"84_16/7/2020 6:30:17 PM","2020-07-09","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Newly fabricated fresh waterline flanges at many places fixed only on 2 bolts.","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","Equipment Related","","","","","Vessel short of correct size of nut bolts. Nut bolts of correct size ordered and received at Singapore, same renewed","2020-07-11","","Completed","2020-07-17","No","No","No","Internal"]
[null,null,null,null,13550,"84_17/7/2020 2:44:07 PM","2020-07-09","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Refman not installed/activated onboard PC, To liaise with PAL helpdesk foe installing on Pcs.","Miscellaneous","Cert. & Docu.","Equipment Related","","","","","Refman installed by Office.","2020-07-19","","Completed","2020-07-15","No","No","No","Internal"]
[null,null,null,null,13551,"84_17/7/2020 3:02:09 PM","2020-07-09","Observation","Owner / Marine / Tech. Suptd.","Engineering Audit","SEWAGE PLANT  BLOWER ERRATIC , TO REPLACE AND OVERHAUL  WITH NEW RECEIVED SPARE","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","REPLACED WITH NEW SPARE.","2020-07-14","","Completed","2020-07-10","No","No","No","External"]
[null,null,null,null,13552,"84_17/7/2020 3:12:15 PM","2020-07-09","Defect","Owner / Marine / Tech. Suptd.","Engineering Audit","ME FO flowmeter erratic, to overhaul & check, if required raise RFQ for required parts","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","MADE OPERATIONAL","2020-07-24","","Completed","2020-07-12","No","No","No","Internal"]
[null,null,null,null,13553,"84_17/7/2020 3:15:56 PM","2020-07-09","Critical Equipment","Owner / Marine / Tech. Suptd.","Engineering Audit","Emg air compressor bottle filled only upto 18 bar, mark the max pressure on the gauge & put notice to fill at required pressure at all times.","Critical Equip.","Eng. / Strg. Comp.","Inappropriate Procedure","10.16","Very High","","","COMPLETED","2020-07-10","","Completed","2020-07-10","No","No","No","Internal"]
[null,null,null,null,13554,"84_17/7/2020 3:18:58 PM","2020-07-09","Observation","Owner / Marine / Tech. Suptd.","Engineering Audit","Quick closing v/v air bottle has a lot of condensed water from drain, to out notice” drain every 2 days & prior using the bottle air","Critical Equip.","Eng. / Strg. Comp.","Inappropriate Procedure","10.16","Very High","","","NOTICE PUT ON QUICK CLOSING VALVE AIR BOTTLE.","2020-07-11","","Completed","2020-07-10","No","No","No","Internal"]
[null,null,null,null,13555,"84_17/7/2020 3:24:22 PM","2020-07-09","Observation","Owner / Marine / Tech. Suptd.","Engineering Audit","ME stuffing box to secure with studs as per manual instruction, presently secured in incorrect way","E/R - Main Engine","Eng. / Strg. Comp.","Inappropriate Procedure","","","","","COMPLETED, TOOL IN PLACE","2020-07-24","","Completed","2020-07-14","No","No","No","Internal"]
[null,null,null,null,13556,"84_17/7/2020 3:33:46 PM","2020-07-09","Other","Owner / Marine / Tech. Suptd.","Engineering Audit","Vessel is not maintaining register of daily sounding of DB tanks & ME sump tank, same to be made with immediate effect & sounding to be taken twice a day","Documentation","Cert. & Docu.","Inappropriate Procedure","","","","","LOGs maintained","2020-07-10","","Completed","2020-07-10","No","No","No","Internal"]
[null,null,null,null,13557,"84_17/7/2020 3:41:43 PM","2020-07-09","Observation","Owner / Marine / Tech. Suptd.","Engineering Audit","Newly received water in oil sensor to be fitted on ME lube oil line","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Fitted in place","2020-07-24","","Completed","2020-07-10","No","No","No","Internal"]
[null,null,null,null,13558,"84_17/7/2020 3:52:09 PM","2020-07-09","Observation","Owner / Marine / Tech. Suptd.","Engineering Audit","Bunker line last stencilled on pipe showing 22 June 19, same has to be carried out annually, carry out pressure test & stencil accordingly","Deck - Pipe / Fittings","Cert. & Docu.","Inappropriate Procedure","6.7","High","","","STENCIL DONE","2020-07-14","","Completed","2020-07-12","No","No","No","Internal"]
[null,null,null,null,13559,"84_17/7/2020 3:48:48 PM","2020-07-09","Observation","Owner / Marine / Tech. Suptd.","Engineering Audit","emergency gen room light tube light fitting with new shade to mark with red dot which are from emergency source","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Inappropriate Procedure","10.36","Very High","","","TO MARK WITH RED DOT","2020-07-12","","Completed","2020-07-10","No","No","No","Internal"]
[null,null,null,null,13560,"84_16/7/2020 6:55:49 PM","2020-07-09","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Stay wire of midship light stands,denzo tape to remove & check the conditions.","Miscellaneous","General Appearance","Equipment Related","","","","","Anti corrosive tape to be renewed and stay wire inspected.","2020-07-24","","Completed","2020-07-28","No","No","No","Internal"]
[null,null,null,null,13561,"84_16/7/2020 6:46:01 PM","2020-07-09","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Stbd side bilge & sewage shore connc. Drip tray channel wasted","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","Equipment Related","","","","","Cold repairs to be carried out & specs to be made in refman for permanent repairs","2020-07-12","","Completed","2020-08-01","No","No","No","Internal"]
[null,null,null,null,13562,"84_17/7/2020 3:38:14 PM","2020-07-09","Observation","Owner / Marine / Tech. Suptd.","Engineering Audit","sewage plant & monthly drinking water onboard test soft copy not maintained onboard, to test & save results on monthly basis","Documentation","Eng. / Strg. Comp.","Inappropriate Procedure","12.8","High","","","Test logs file soft copy is being maintained now.","2020-07-24","","Completed","2020-08-07","No","No","No","Internal"]
[null,null,null,null,13563,"84_17/7/2020 3:21:47 PM","2020-07-09","Observation","Owner / Marine / Tech. Suptd.","Engineering Audit","Both ME air cooler mist catcher side door inspection to carry out at next anchorage as per MAN circular","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Mist catcher inspection carried out","2020-08-09","","Completed","2020-08-10","No","No","No","Internal"]
[null,null,null,null,13565,"84_16/7/2020 6:26:05 PM","2020-07-09","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","7S overfill conduit pipe wasted & holed around 1 mtr.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related",null,null,"Not Applicable","Not Applicable","Cold repairs to be carried out & make specs for permanent repair in Refman","2020-07-19",null,"Completed","2020-08-03","No","No","No","Internal"]
[null,null,null,null,null,"84_5/1/2021 8:45:45 PM","2020-07-09","Observation","Owner / Marine / Tech. Suptd.","Engineering Audit","Both Fire & GS pp & emergency fire pp priming pp clutch not engaging fully, to be adjusted in such way, that in stop condition clutch should always be engaged & once priming carried out/pressure developed it should disengage the clutch. ","E/R - Pumps","Emgcy. Systems","Equipment Related",5.35,"Medium","Not Applicable","Not Applicable","Both fire and GS pump and emergency fire pump cluth were adjusted as per description. Clutch engages at stop condition and disengages after pressure builds up. Overall functioning found satisfactory.","2020-08-31",null,"Completed","2020-07-14","No",null,null,"Internal"]
[null,null,null,null,null,"84_5/1/2021 8:48:35 PM","2020-07-09","Observation","Owner / Marine / Tech. Suptd.","Engineering Audit","Pump room bottom platform 5 in number light shades are cracked, the light fitting to be replaced with new.1 bulb is busted.","Elect. Mach. & Equip.","Cargo / Ballast Systems","Equipment Related",5.18,"High","Not Applicable","Not Applicable","Pump room bottom platform lights replaced with new spare received.","2020-12-31",null,"Completed","2020-12-15","No",null,null,"Internal"]
[null,null,null,null,null,"84_17/7/2020 3:45:33 PM","2020-07-09","Observation","Owner / Marine / Tech. Suptd.","Engineering Audit","ME Aft air cooler around 72 tubes are hard to clean, vessel to carry out chemical circulation & then use queue machine to clear the tubes in case if there is high scav temperature. during passage to next port","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","ME cooler elements cleaned mechanicaly by brush and chemical. Tubes were cleared and found performance of cooler satisfactory.","2021-08-31",null,"Completed","2020-12-30","No",null,null,"Internal"]
[null,null,null,null,null,"84_16/1/2021 4:54:11 PM","2020-07-09","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","steering gear oil storage tank though above min level, to top up till max tank level for using in emergency.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related",10.4,"Medium","Not Applicable","Not Applicable","Oil storage tank filled up to the max tank level.","2020-07-15",null,"Completed","2020-07-11","No",null,null,"Internal"]
[null,null,null,null,13542,"84_17/7/2020 11:12:49 AM","2020-07-13","Defect","Ship Staff","Engineering Audit","BOILER GAUGE-GLASS STEAM SIDE VALVE BONNET - GASKET LEAK","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","Repaired by lapping the seating surface of the valve bonnet and putting extra gasket. Now no leak","2020-09-12","","Completed","2020-09-11","No","No","No","Internal"]
[null,null,null,null,13564,"84_17/7/2020 8:41:23 AM","2020-07-15","Observation","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","The vessel SPM arrangement was noted with the angle of change of direction of the pick-up line was large, with an aggregate of all changes approx 180 degrees.","Deck - Pipe / Fittings","Mooring","Equipment Related","9.26","Low","","","This is design of the vessel from shipyard. Same has been approved by Class. ","2020-07-15","","Completed","2020-07-15","No","No","No","External"]
[null,null,null,null,null,"84_17/7/2020 8:53:37 AM","2020-07-15","Observation","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","The SDMBL was declared as 79T, however, the LDBF were noted ranging from I01 T to\r\n\r\n109.9T for the 16 mooring wires in use, which was ranging from 128% to 139%, instead of 100% to 105% whilst the TDBF were noted ranging from 131 T to 161.2T for the 14 tail ropes in use, which was ranging from 165% to 204% instead of 125% to 130% as per MEG 5.2.1.","Miscellaneous","Mooring","Equipment Related",9.5,"High","Not Applicable","Not Applicable","Wires/ Tails  being renewed as per requirement of MEG4 in a phased manner.7 wires and 9 tails renewed and complying with MEG4 which were received at Fujairah on 06-Dec-2020.","2021-05-31",null,"Completed","2020-12-28","No",null,null,"External"]
[null,null,null,null,null,"84_12/8/2020 7:00:51 PM","2020-08-05","Defect","Ship Staff","Engineering Audit","Steering gear motor chain coupling - chain links have developed some dents and there is more play in roller pins and its bushing.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related",null,null,"Not Applicable","Not Applicable","chain couplings renewed with spares received","2021-02-28",null,"Completed","2021-01-09","No",null,null,"Internal"]
[null,null,null,null,null,"84_12/8/2020 7:04:33 PM","2020-08-08","Defect","Ship Staff","Engineering Audit","Rocker arm shaft for no.1 DG no.1 unit has worn out. Same needs to be renewed.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related",null,null,"Not Applicable","Not Applicable","Shaft changed with new spare received. Engine tried out and all found satisfactory.","2020-11-07",null,"Completed","2020-12-27","No",null,null,"Internal"]
[null,null,null,null,null,"84_16/11/2020 11:24:11 AM","2020-10-05","Defect","Ship Staff","Ship Staff Insp.","1P COT Main Valve suspected leaking.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related",8.14,"Very High","Not Applicable","Not Applicable","Leak rectified.Same to be checked and monitored during next operation.","2020-12-31",null,"Completed","2020-12-26","No",null,null,"Internal"]
[null,null,null,null,null,"84_12/10/2020 10:36:36 PM","2020-10-06","Defect","Ship Staff","Ship Staff Insp.","Steam Line to 1P COT found Corroded and wasted.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related",11.4,"Very High","Not Applicable","Not Applicable","Pipe fabricated and replaced. Line tested during discharging, found in good order.","2020-11-30",null,"Completed","2020-11-19","No",null,null,"Internal"]
[null,null,null,null,null,"84_1/11/2020 10:14:04 PM","2020-10-06","Defect","Ship Staff","Ship Staff Insp.","Speed Log Giving erratic reading at Times.","Navigation - Echo Sounder / Speed Log","Navigation","Equipment Related",null,null,"Not Applicable","Not Applicable","Speed Log Sensor cleaned and fitted back.Presently showing correct readings","2020-12-31",null,"Completed","2020-12-20","Yes",null,null,"Internal"]
[null,null,null,null,null,"84_12/10/2020 10:39:29 PM","2020-10-10","Defect","Ship Staff","Ship Staff Insp.","Steam Branch Line to 3P COT found wasted and corroded at few sections under the U Clamp.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related",11.4,"Very High","Not Applicable","Not Applicable","Corroded section replaced with a newly fabricated section.","2020-11-30",null,"Completed","2020-11-19","No",null,null,"Internal"]
[null,null,null,null,null,"84_31/10/2020 3:48:12 PM","2020-10-16","Defect","Ship Staff","Ship Staff Insp.","On inspection found hose handling crane sheave rusted and not rotating on bearing and pin.","Deck - Machinery","Cargo / Ballast Systems","Equipment Related,Inappropriate Procedure",null,null,"Not Applicable","Not Applicable","Sheave taken out and corroded/wasted area was built up by welding in workshoip. Bearings cleaned and grease renewed. Sheave put back and crane tried out. Sheave now rotating freely.","2020-10-21",null,"Completed","2020-10-21","No",null,null,"Internal"]
[null,null,null,null,14355,"84_31/10/2020 3:39:46 PM","2020-10-23","Observation","Ship Staff","Ship Staff Insp.","COP no.3 while running observed lower bearing temperature rising to 75 degree.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","Bottom bearing inspected and found housing wear down. punch marks are made and fitted new bearing. Pump tried out and found temperature steady at u58 deg celcius.","2020-10-31","","Completed","2020-11-03","No","No","No","Internal","Please revert with update on progress status for same."]
[null,null,null,null,16043,"84_05/11/2020 11:47:00 AM","2020-10-27","Defect","Ship Staff","Ship Staff Insp.","Hydraulic return line for fwd spring winch found rusted and leaking.","Deck - Pipe / Fittings","Mooring","Equipment Related","11.4","Very High","","","New pipeline fabricated and installed.","2020-11-30","","Completed","2020-10-30","No","No","No","Internal"]
[null,null,null,null,null,"84_30/11/2020 12:46:04 PM","2020-11-28","Breakdown","Ship Staff","Ship Staff Insp.","Main air compressor no. 2 found cranckcase pressurized. On opening and inspection found piston broken.","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related",null,null,"Not Applicable","Not Applicable","Brocken piston replaced with overhauled old spare with new piston rings and scrapper rings. All clearances taken and found within limits. Compressor tried out working satisfactory.","2020-12-04",null,"Completed","2020-11-30","No",null,null,"Internal"]

{"sheet":"Calc","index":2,"n_rows":28,"n_cols":12,"rows_kept":28,"cut":false,"hidden":true,"merged":[]}
["Def_type","Def_cause","Equipments","VIQrefno","Observer_code"]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,"Dim itemSele As Long"]
[null,null,null,null,null,null,null,null,null,null,null,"   dim startRow as integer"]
[null,null,null,null,null,null,null,null,null,null,null,"   startRow=1"]
[null,null,null,null,null,null,null,null,null,null,null,"        For itemSele = 0 To ListBox1.ListCount - 1"]
[null,null,null,null,null,null,null,null,null,null,null,"        If ListBox1.Selected(itemSele) = True Then"]
[null,null,null,null,null,null,null,null,null,null,null,"        Worksheets(\"WorksheetName\").Range(\"A\" & startRow).Value = ListBox1.List(itemSele)"]
[null,null,null,null,null,null,null,null,null,null,null,"        startRow = startRow + 1"]
[null,null,null,null,null,null,null,null,null,null,null,"        End If"]
[null,null,null,null,null,null,null,null,null,null,null,"        Next"]
[null,null,null,null,null,null,null,null,null,null,null,"Dim LastRowA As String"]
[null,null,null,null,null,null,null,null,null,null,null,"        Dim itemSele As Long"]
[null,null,null,null,null,null,null,null,null,null,null,"       Dim startRow as integer"]
[null,null,null,null,null,null,null,null,null,null,null,"        LastRowA = ActiveSheet.Cells(Rows.count, \"A\").End(xlUp).row"]
[null,null,null,null,null,null,null,null,null,null,null,"        startQue = 0"]
[null,null,null,null,null,null,null,null,null,null,null,"        For itemSele = 0 To ListBox1.ListCount - 1"]
[null,null,null,null,null,null,null,null,null,null,null,"        For startRow = 1 To LastRowA"]
[null,null,null,null,null,null,null,null,null,null,null,"        If Worksheets(\"WorksheetName\").Range(\"A\" & startRow).Value = ListBox1.List(itemSele) Then"]
[null,null,null,null,null,null,null,null,null,null,null,"        ListBox1.Selected(itemSele) = True"]
[null,null,null,null,null,null,null,null,null,null,null,"        Exit For"]
[null,null,null,null,null,null,null,null,null,null,null,"        End If"]
[null,null,null,null,null,null,null,null,null,null,null,"        Next j"]
[null,null,null,null,null,null,null,null,null,null,null,"        Next"]
[null,null,null,null,null,null,null,null,null,null,null,"        End If"]

{"sheet":"Areaofobs","index":3,"n_rows":17,"n_cols":2,"rows_kept":17,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Cargo / Ballast Systems",11]
["Cert. & Docu.",2]
["Communication",6]
["Crew Management",3]
["Emgcy. Systems",13]
["Eng. / Strg. Comp.",14]
["General Appearance",15]
["Ice Opns.",17]
["ISM Related",7]
["ISPS Related",10]
["MARPOL Related",9]
["MLC Related",4]
["Mooring",12]
["Navigation",5]
["Safety / LSA / FFA",8]
["Structural Condn. / WT integrity ",16]

{"sheet":"Vessel_type","index":4,"n_rows":1,"n_cols":2,"rows_kept":1,"cut":false,"hidden":true,"merged":[]}
["Vessel_type","ID"]

{"sheet":"Deficiency_type","index":5,"n_rows":8,"n_cols":3,"rows_kept":8,"cut":false,"hidden":true,"merged":[]}
["TITLE","Type of deficiency_description","ID"]
["Breakdown",null,6]
["Critical Equipment",null,4]
["Defect",null,1]
["Guarantee Claim",null,8]
["Non Conformity",null,2]
["Observation",null,3]
["Other",null,7]

{"sheet":"VIQrefno","index":6,"n_rows":427,"n_cols":3,"rows_kept":427,"cut":false,"hidden":true,"merged":[]}
["VIQ_ref_no","Risk Value of observation","ID"]
["1.1","Low",8243]
["1.10","Low",8252]
["1.11","Low",8253]
["1.12","Low",8254]
["1.13","Low",8255]
["1.14","Low",8256]
["1.15","Low",8257]
["1.16","Low",8259]
["1.17","Low",8260]
["1.18","Low",8261]
["1.19","Low",8262]
["1.2","Low",8244]
["1.20","Low",8263]
["1.21","Low",8265]
["1.22","Low",8266]
["1.23","Low",8267]
["1.24","Low",8268]
["1.25","Low",8269]
["1.26","Low",8270]
["1.3","Low",8245]
["1.4","Low",8246]
["1.5","Low",8247]
["1.6","Low",8248]
["1.7","Low",8249]
["1.8","Low",8250]
["1.9","Low",8251]
["1.99","High",11258]
["10.1","Medium",8461]
["10.10","High",8470]
["10.11","Medium",8471]
["10.12","Very High",8472]
["10.13","Very High",8473]
["10.14","Medium",8474]
["10.15","Low",8475]
["10.16","Very High",8476]
["10.17","Very High",8477]
["10.18","High",8478]
["10.19","Very High",8479]
["10.2","Low",8462]
["10.20","High",8480]
["10.21","Medium",8481]
["10.22","Low",8482]
["10.23","Medium",8483]
["10.24","Low",8484]
["10.25","Very High",8485]
["10.26","High",8486]
["10.27","Medium",8487]
["10.28","Low",8488]
["10.29","Medium",8489]
["10.3","Medium",8463]
["10.30","High",8490]
["10.31","Very High",8491]
["10.32","Very High",8492]
["10.33","High",8493]
["10.34","High",8494]
["10.35","Very High",8495]
["10.36","Very High",8496]
["10.37","Medium",8497]
["10.38","Medium",8498]
["10.39","High",8499]
["10.4","High",8464]
["10.40","Medium",8500]
["10.41","Medium",8501]
["10.42","Medium",8502]
["10.43","Medium",8503]
["10.44","Medium",8504]
["10.45","Very High",8505]
["10.46","High",8506]
["10.47","Medium",8507]
["10.48","High",8508]
["10.49","Medium",8509]
["10.5","Low",8465]
["10.50","High",8510]
["10.51","Low",8511]
["10.52","Medium",8512]
["10.53","Medium",8513]
["10.54","High",8514]
["10.55","Low",8515]
["10.6","Very High",8466]
["10.7","Medium",8467]
["10.8","Medium",8468]
["10.9","Medium",8469]
["10.99","High",8516]
["11.1","High",8420]
["11.10","Medium",8429]
["11.11","Very High",8430]
["11.12","Low",8431]
["11.13","Low",8432]
["11.14","Medium",8433]
["11.15","Low",8434]
["11.16","Low",8435]
["11.17","Low",8436]
["11.2","Medium",8421]
["11.3","Medium",8422]
["11.4","Very High",8423]
["11.5","Medium",8424]
["11.6","Medium",8425]
["11.7","High",8426]
["11.8","Low",8427]
["11.9","Low",8428]
["11.99","High",8437]
["12.1","High",8438]
["12.10","High",8448]
["12.11","High",8449]
["12.12","High",8450]
["12.13","High",8451]
["12.14","High",8452]
["12.15","High",8453]
["12.16","High",8454]
["12.17","High",8455]
["12.18","High",8456]
["12.19","High",8457]
["12.2","High",8439]
["12.20","High",8458]
["12.21","High",8459]
["12.3","High",8441]
["12.4","High",8442]
["12.5","High",8443]
["12.6","High",8444]
["12.7","High",8445]
["12.8","High",8446]
["12.9","High",8447]
["12.99","High",8460]
["2.1","Very High",8296]
["2.1.9","Very High",11259]
["2.10","Medium",8304]
["2.11","Medium",8305]
["2.12","Low",8306]
["2.13","Low",8307]
["2.14","Low",8308]
["2.15","Low",8309]
["2.16","Medium",8310]
["2.2","Medium",8297]
["2.3","High",8295]
["2.4","Medium",8298]
["2.5","Medium",8299]
["2.6","Low",8300]
["2.7","High",8301]
["2.8","High",8302]
["2.9","Medium",8303]
["2.99","High",8311]
["3.1","High",8312]
["3.2","Very High",8313]
["3.3","High",8314]
["3.4","Low",8294]
["3.5","Medium",8315]
["3.6","High",8316]
["3.7","Very High",8317]
["3.8","Very High",8318]
["3.99","High",8319]
["4.1","High",8320]
["4.10","High",8329]
["4.11","Medium",8330]
["4.12","Very High",8331]
["4.13","Very High",8332]
["4.14","Very High",8333]
["4.15","Very High",8334]
["4.16","Very High",8335]
["4.17","Very High",8336]
["4.18","Very High",8337]
["4.19","Low",8338]
["4.2","Medium",8321]
["4.20","Very High",8339]
["4.21","High",8340]
["4.22","Low",8341]
["4.23","High",8342]
["4.24","High",8343]
["4.25","Low",8344]
["4.26","Low",8345]
["4.27","High",8346]
["4.3","Medium",8322]
["4.4","High",8323]
["4.5","Very High",8324]
["4.6","Medium",8325]
["4.7","High",8326]
["4.8","Medium",8327]
["4.9","Medium",8328]
["4.99","High",8347]
["5.1","Very High",8517]
["5.10","High",8526]
["5.11","Low",8527]
["5.12","Medium",8528]
["5.13","High",8529]
["5.14","Very High",8530]
["5.15","Medium",8531]
["5.16","Very High",8532]
["5.17","Very High",8533]
["5.18","High",8534]
["5.19","Medium",8535]
["5.2","Very High",8518]
["5.20","Medium",8536]
["5.21","Medium",8537]
["5.22","High",8539]
["5.23","Very High",8540]
["5.24","Very High",8541]
["5.25","Medium",8542]
["5.26","Medium",8543]
["5.27","Medium",8544]
["5.28","Very High",8545]
["5.29","High",8546]
["5.3","Low",8519]
["5.30","High",8547]
["5.31","High",8548]
["5.32","High",8549]
["5.33","High",8550]
["5.34","Low",8551]
["5.35","Medium",8552]
["5.36","Low",8553]
["5.37","Low",8554]
["5.38","High",8555]
["5.39","Very High",8556]
["5.4","High",8520]
["5.40","Very High",8557]
["5.41","Very High",8558]
["5.42","Medium",8559]
["5.43","High",8560]
["5.44","High",8561]
["5.45","Medium",8564]
["5.46","Medium",8565]
["5.47","Medium",8566]
["5.48","Medium",8567]
["5.5","Low",8521]
["5.6","Low",8522]
["5.7","Medium",8523]
["5.8","Medium",8524]
["5.9","Very High",8525]
["5.99","High",8568]
["6.1","Medium",8348]
["6.10","Low",8357]
["6.11","High",8358]
["6.12","Medium",8359]
["6.13","Low",8360]
["6.14","High",8361]
["6.15","High",8362]
["6.16","Very High",8363]
["6.17","Very High",8364]
["6.18","Medium",8365]
["6.19","Low",8366]
["6.2","High",8349]
["6.20","Medium",8367]
["6.21","High",8368]
["6.22","Medium",8369]
["6.3","Low",8350]
["6.4","High",8351]
["6.5","Medium",8352]
["6.6","Medium",8353]
["6.7","High",8354]
["6.8","High",8355]
["6.9","Low",8356]
["6.99","High",8370]
["7.1","High",8371]
["7.10","High",8380]
["7.11","High",8381]
["7.12","High",8382]
["7.13","Medium",8383]
["7.14","Medium",8384]
["7.15","High",8385]
["7.16","High",8386]
["7.17","High",8387]
["7.2","High",8372]
["7.3","Low",8373]
["7.4","Low",8374]
["7.5","Low",8375]
["7.6","Medium",8376]
["7.7","Low",8377]
["7.8","High",8378]
["7.9","High",8379]
["7.99","High",8388]
["8.1","Very High",8569]
["8.10","Very High",8578]
["8.100","Low",11227]
["8.101","Medium",11228]
["8.102","Low",11229]
["8.103","Low",11230]
["8.104","Low",11231]
["8.105","Medium",11232]
["8.106","Medium",11233]
["8.107","Low",11234]
["8.108","High",11235]
["8.109","Very High",11236]
["8.11","Medium",8579]
["8.110","High",11237]
["8.111","Medium",11238]
["8.112","High",11239]
["8.113","Medium",11240]
["8.114","Low",11241]
["8.115","High",11242]
["8.116","Medium",11243]
["8.117","Medium",11244]
["8.118","Medium",11245]
["8.119","High",11246]
["8.12","Medium",8580]
["8.120","High",11247]
["8.121","Medium",11248]
["8.122","High",11249]
["8.123","High",11250]
["8.124","Low",11251]
["8.125","High",11252]
["8.126","Medium",11253]
["8.127","Medium",11254]
["8.13","Medium",8581]
["8.14","Very High",8582]
["8.15","High",8583]
["8.16","Very High",8584]
["8.17","Low",8585]
["8.18","High",8586]
["8.19","High",8587]
["8.199","High",11255]
["8.2","Medium",8570]
["8.20","Medium",8588]
["8.21","High",8589]
["8.22","Very High",8590]
["8.23","Medium",8591]
["8.24","Medium",8592]
["8.25","Very High",8593]
["8.26","High",8594]
["8.27","Medium",8595]
["8.28","Medium",8596]
["8.29","High",8598]
["8.3","Very High",8571]
["8.30","High",8599]
["8.31","High",8600]
["8.32","Low",8601]
["8.33","Medium",8602]
["8.34","High",8603]
["8.35","Medium",8604]
["8.36","Medium",8605]
["8.37","High",8607]
["8.38","Medium",8608]
["8.39","Medium",8609]
["8.4","Medium",8572]
["8.40","High",8610]
["8.41","Medium",8611]
["8.42","Medium",8612]
["8.43","Very High",8613]
["8.44","High",8615]
["8.45","High",8616]
["8.46","Very High",8617]
["8.47","Very High",8618]
["8.48","Medium",8619]
["8.49","High",8620]
["8.5","Very High",8573]
["8.50","Medium",8621]
["8.51","Low",8622]
["8.52","Low",8623]
["8.53","Low",8624]
["8.54","High",8625]
["8.55","Low",11182]
["8.56","Medium",11183]
["8.57","Medium",11184]
["8.58","High",11185]
["8.59","High",11186]
["8.6","Medium",8574]
["8.60","High",11187]
["8.61","Medium",11188]
["8.62","Very High",11189]
["8.63","High",11190]
["8.64","Medium",11191]
["8.65","Low",11192]
["8.66","High",11193]
["8.67","High",11194]
["8.68","High",11195]
["8.69","Medium",11196]
["8.7","High",8575]
["8.70","Medium",11197]
["8.71","Very High",11198]
["8.72","Medium",11199]
["8.73","Medium",11200]
["8.74","High",11201]
["8.75","Medium",11202]
["8.76","Medium",11203]
["8.77","Medium",11204]
["8.78","Medium",11205]
["8.79","Medium",11206]
["8.8","Medium",8576]
["8.80","Medium",11207]
["8.81","Low",11208]
["8.82","Medium",11209]
["8.83","Low",11210]
["8.84","Low",11211]
["8.85","Medium",11212]
["8.86","Medium",11213]
["8.87","Medium",11214]
["8.88","Low",11215]
["8.89","High",11216]
["8.9","High",8577]
["8.90","High",11217]
["8.91","High",11218]
["8.92","Medium",11219]
["8.93","Low",11220]
["8.94","Low",11221]
["8.95","Medium",11222]
["8.96","Medium",11223]
["8.97","Low",11224]
["8.98","High",11225]
["8.99","Medium",11226]
["9.1","Low",8390]
["9.10","Medium",8399]
["9.11","Medium",8400]
["9.12","Medium",8401]
["9.13","Low",8402]
["9.14","Medium",8403]
["9.15","Medium",8404]
["9.16","High",8405]
["9.17","High",8406]
["9.18","Low",8407]
["9.19","Low",8408]
["9.2","Very High",8391]
["9.20","Medium",8409]
["9.21","Medium",8410]
["9.22","Low",8411]
["9.23","Low",8412]
["9.24","Medium",8413]
["9.25","Low",8414]
["9.26","Low",8415]
["9.27","Low",8416]
["9.28","Medium",8417]
["9.29","Low",8418]
["9.3","Very High",8392]
["9.4","High",8393]
["9.5","High",8394]
["9.6","Low",8395]
["9.7","Medium",8396]
["9.8","Medium",8397]
["9.9","Medium",8398]
["9.99","High",8419]

{"sheet":"Equipment_list","index":7,"n_rows":28,"n_cols":3,"rows_kept":28,"cut":false,"hidden":true,"merged":[]}
["TITLE","Equipment_list_description","ID"]
["Accommodation",null,12]
["Cargo Mach.",null,13]
["Critical Equip.",null,16]
["Deck - Machinery",null,18]
["Deck - Mooring Machinery",null,15]
["Deck - Pipe / Fittings",null,20]
["Documentation",null,21]
["E/R - Air Comp.",null,8]
["E/R - Aux. Engine",null,4]
["E/R - Aux. Mach.",null,7]
["E/R - Boiler",null,5]
["E/R - Main Engine",null,3]
["E/R - Pipes/ valves & fittings",null,9]
["E/R - Pumps",null,32]
["E/R - Purifier",null,6]
["Elect. Mach. & Equip.",null,10]
["Hull & Tanks",null,19]
["Inert Gas",null,14]
["LSA / FFA",null,17]
["Miscellaneous",null,22]
["Navigation - DGPS / EPFS / AIS",null,28]
["Navigation - ECDIS",null,25]
["Navigation - Echo Sounder / Speed Log",null,26]
["Navigation - GMDSS & Communication",null,23]
["Navigation - Others",null,11]
["Navigation - RADAR",null,24]
["Navigation - VDR / BNWAS",null,30]

{"sheet":"PSC_MOU","index":8,"n_rows":11,"n_cols":3,"rows_kept":11,"cut":false,"hidden":true,"merged":[]}
["TITLE","PSC_MOU_description","ID"]
["Asia and the Pacific",null,2]
["Caribbean",null,4]
["Europe and the North Atlantic",null,1]
["Latin America",null,3]
["The Black Sea region",null,6]
["The Indian Ocean",null,8]
["The Mediterranean",null,7]
["The Riyadh MoU",null,9]
["USCG",null,10]
["West and Central Africa",null,5]

{"sheet":"Inspection_type","index":9,"n_rows":13,"n_cols":2,"rows_kept":13,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Bunkering Audit",14]
["Cargo Audit",17]
["Engineering Audit",16]
["ISM Audit",2]
["ISPS Audit",3]
["IT Audit",10]
["MLC Audit",1]
["Mooring Audit",9]
["Nav Audit / Verification",8]
["Onboard Training",18]
["Ship Staff Insp.",15]
["Suptd. Insp.",13]

{"sheet":"Deficiency_Cause","index":10,"n_rows":8,"n_cols":3,"rows_kept":8,"cut":false,"hidden":true,"merged":[]}
["TITLE","Deficiency_Cause_description","ID"]
["Behaviour Based",null,1]
["Equipment Related",null,4]
["External Factors",null,5]
["Human Error",null,7]
["Inappropriate Procedure",null,8]
["Industry Issue",null,6]
["Knowledge Based",null,3]

{"sheet":"Observer_code","index":11,"n_rows":3,"n_cols":3,"rows_kept":3,"cut":false,"hidden":true,"merged":[]}
["TITLE","Observer_code_description","ID"]
["Owner / Marine / Tech. Suptd.",null,3]
["Ship Staff",null,2]

{"sheet":"Status_code","index":12,"n_rows":6,"n_cols":3,"rows_kept":6,"cut":false,"hidden":true,"merged":[]}
["TITLE","Status_code_description","ID"]
["Completed",null,6]
["Deferred to D D",null,5]
["In progress",null,3]
["Not Started",null,2]
["Waiting spare",null,4]

{"sheet":"PSC_ref_no","index":13,"n_rows":19,"n_cols":2,"rows_kept":19,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Alarms",9]
["Cargo operations including equipment",7]
["Certificates & Documentation",2]
["Dangerous Goods",13]
["Emergency Systems",5]
["Fire safety",8]
["ISM",16]
["ISPS",17]
["Life saving appliances",12]
["MLC, 2006",18]
["Other",19]
["Pollution Prevention",15]
["Propulsion and auxiliary machinery",14]
["Radio communication",6]
["Safety of Navigation",11]
["Structural condition",3]
["Water/Weathertight condition",4]
["Working and Living Conditions",10]

{"sheet":"Risk_value_of_obs","index":14,"n_rows":1,"n_cols":2,"rows_kept":1,"cut":false,"hidden":true,"merged":[]}
["Risk Value of observation","ID"]

{"sheet":"Year","index":15,"n_rows":18,"n_cols":1,"rows_kept":18,"cut":false,"hidden":true,"merged":[]}
["Year"]
[2014]
[2015]
[2016]
[2017]
[2018]
[2019]
[2020]
[2021]
[2022]
[2023]
[2024]
[2025]
[2026]
[2027]
[2028]
[2029]
[2030]

{"sheet":"Month","index":16,"n_rows":13,"n_cols":1,"rows_kept":13,"cut":false,"hidden":true,"merged":[]}
["Month"]
["Jan"]
["Feb"]
["Mar"]
["Apr"]
["May"]
["Jun"]
["Jul"]
["Aug"]
["Sep"]
["Oct"]
["Nov"]
["Dec"]

{"sheet":"Date_","index":17,"n_rows":32,"n_cols":1,"rows_kept":32,"cut":false,"hidden":true,"merged":[]}
["Date"]
["01"]
["02"]
["03"]
["04"]
["05"]
["06"]
["07"]
["08"]
["09"]
[10]
[11]
[12]
[13]
[14]
[15]
[16]
[17]
[18]
[19]
[20]
[21]
[22]
[23]
[24]
[25]
[26]
[27]
[28]
[29]
[30]
[31]

{"sheet":"Sheet1","index":18,"n_rows":24,"n_cols":6,"rows_kept":24,"cut":false,"hidden":true,"merged":[]}
[]
[null,"ID","E",null,"Date Recorded",1]
[null,"UNIQUE ID","F",null,"Type of Deficiency",2]
[1,"Date Recorded","G",null,"Observer code",3]
["ignore","Vessel Type","H",null,"Type of Inspection",4]
[null,"Internal / External","I",null,"Description of Deficiency",5]
[null,"Drydock","J",null,"Equipment Categories",6]
[null,"Information Sharing","K",null,"Area of Observation",7]
[null,"Critical_item","L",null,"Deficiency Cause",8]
[null,"Deficiency Type","M",null,"VIQ Ref Number",9]
[null,"Deficiency Cause","N",null,"Risk Value of Obs",10]
[null,"Inspection Type","O",null,"PSC Ref Number",11]
[null,"Equipments","P",null,"PSC MOU ID",12]
[null,"VIQ Reference Number","Q",null,"Action Taken or Required",13]
[null,"Risk Value of the observation","R",null,"Target Date",14]
[null,"PSC Reference Number","S",null,"PO Ref No.",15]
[null,"PSC MOU","T",null,"Status Code",16]
[null,"Observer Code","U",null,"Date Completed",17]
[null,"Target Date","V",null,"Drydock",18]
[null,"Status Code","W",null,"Info Sharing",19]
[null,"Description of Deficiency","X",null,"Critical Item Flag",20]
[null,"Action taken / required","Y",null,"Audit Type",21]
[null,"PO ref no","Z"]
[null,"Date completed","AA"]

{"sheet":"Ship_information","index":19,"n_rows":2,"n_cols":3,"rows_kept":2,"cut":false,"hidden":true,"merged":[]}
["Ship_ID","Ship_Name","FILE_NAME"]
["84","A MELODY (24-12-2020)","84_1608781927089.xlsm"]

{"sheet":"External_Deficiency_type","index":20,"n_rows":5,"n_cols":3,"rows_kept":5,"cut":false,"hidden":true,"merged":[]}
["TITLE","Type of deficiency_description","ID"]
["Condn of Class / Memo",null,5]
["Defect",null,1]
["Non Conformity",null,2]
["Observation",null,3]

{"sheet":"External_Inspection_type","index":21,"n_rows":11,"n_cols":2,"rows_kept":11,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Cargo Audit",17]
["Flag State Insp.",5]
["ISM Audit",2]
["ISPS Audit",3]
["MLC Audit",1]
["Nav Audit / Verification",8]
["OM Insp. (Eg. SIRE / CDI etc.)",6]
["Others (Eg. Insurance etc.)",12]
["PSC Inspection",4]
["Terminal Insp.",11]

{"sheet":"External_Observer_code","index":22,"n_rows":7,"n_cols":3,"rows_kept":7,"cut":false,"hidden":true,"merged":[]}
["TITLE","Observer_code_description","ID"]
["Class Surveyor",null,4]
["FSC Inspector",null,5]
["Others (Eg. Insurance etc.)",null,9]
["PSC Insp.",null,6]
["SIRE / CDI Insp.",null,8]
["Terminal Insp.",null,7]

{"sheet":"Sheet Version","index":23,"n_rows":2,"n_cols":2,"rows_kept":2,"cut":false,"hidden":true,"merged":[]}
["Version","Title"]
["2.0","Version 2.0"]