{"text_format":"1","workbook":"xlsx","n_sheets":24,"sheets":["Mainsheet","Completed","Calc","Areaofobs","Vessel_type","Deficiency_type","VIQrefno","Equipment_list","PSC_MOU","Inspection_type","Deficiency_Cause","Observer_code","Status_code","PSC_ref_no","Risk_value_of_obs","Year","Month","Date_","Sheet1","Ship_information","External_Deficiency_type","External_Inspection_type","External_Observer_code","Sheet Version"],"not_rendered":{"charts":0,"images":5,"macros":1,"external_links":0,"defined_names":12,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Mainsheet","index":0,"n_rows":23,"n_cols":28,"rows_kept":23,"cut":false,"hidden":false,"merged":[[10,8,10,9],[10,12,10,13],[12,6,12,27],[8,6,8,27]]}
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,"Defect - Damage Monitoring Sheet"]
[]
[null,null,null,null,null,null,null,"Date of Report","26-Apr-2021",null,null,"Ship Name","DHT STALLION (26-04-2021)"]
[]
[null,null,null,null,null,null,"VERSION : 2.0"]
[]
[]
[]
[null,null,null,null,"ID","UNIQUE ID","Date Recorded","Type of Deficiency","Observer code","Type of Inspection","Description of Deficiency","Equipment Categories","Area of Observation","Deficiency Cause","VIQ Ref Number","Risk Value of Obs","PSC Ref Number","PSC MOU ID","Action Taken or Required","Target Date","PO Ref No.","Status Code","Date Completed","Drydock","Info Sharing","Critical Item","Audit Type","Superintendent Remarks"]
[null,null,null,null,5612,"57_27/10/2019 8:26:33 AM","2021-01-24","Defect","Ship Staff","Ship Staff Insp.","Vessel Call Sign to be changed to new Call Sign VRSX9 in BWTS Software System from the makers.","Elect. Mach. & Equip.","Cargo / Ballast Systems","Equipment Related","8.18","High","","","Awaiting Maker to  access BWTS monitor by remote access( by internet) and change the Call Sign.","2021-05-30","","Not Started",null,"No","No","No","Internal","Since the maker tried remote access and unable to do because of slow internet speed, it has to be done at next service by maker."]
[null,null,null,null,18742,"57_14/4/2021 2:35:55 PM","2021-03-25","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ODME pressure switch diaphragm damaged and leakage occured.","Critical Equip.","MARPOL Related","Equipment Related","6.13","Low","","","Pressure switch to be renewed. Though ODME is working normally.","2021-07-25","DSTA210086","Waiting spare",null,"No","No","No","Internal","Spare will be supplied next call Singapore."]
[null,null,null,null,18475,"57_31/3/2021 2:30:19 PM","2021-03-30","Defect","Ship Staff","Ship Staff Insp.","Incinerator waste oil settling tank No-1 and No-2 steam extraction fan seals are leaking","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.1","Medium","","","Need to replace seals and bearings on steam extraction fans (vessel does not have spare seals for extraction fan, Requisition DSTA210083 raised)","2021-06-30","DSTA210083","Waiting spare",null,"No","No","No","Internal","Noted."]
[null,null,null,null,18743,"57_12/4/2021 00:40:44","2021-04-07","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Spot rust on port pump room exhaust vent.","Miscellaneous","General Appearance","Equipment Related","11.3","Medium","","","Will be planned in upcoming month maintenance","2021-05-22","","Not Started",null,"No","No","No","Internal","Update progress on weekly deck maintenance report."]
[null,null,null,null,18744,"57_12/4/2021 00:45:26","2021-04-07","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Spot rust on Port and Stbd cargo manifold tray","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.3","Medium","","","Will be planned in upcoming months","2021-05-22","","Not Started",null,"No","No","No","Internal","Update progress on weekly deck maintenance report."]
[null,null,null,null,18745,"57_12/4/2021 00:48:18","2021-04-07","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Spot rust on pipe supports on main deck.","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.7","High","","","Will be planned in upcoming months","2021-06-07","","Not Started",null,"No","No","No","Internal","Update progress on weekly deck maintenance report."]

{"sheet":"Completed","index":1,"n_rows":211,"n_cols":28,"rows_kept":211,"cut":false,"hidden":false,"merged":[[10,8,10,9],[10,12,10,13],[12,6,12,27],[8,6,8,27]]}
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,"Defect - Damage Monitoring Sheet"]
[]
[null,null,null,null,null,null,null,"Date of Report","26-Apr-2021",null,null,"Ship Name","DHT STALLION (26-04-2021)"]
[]
[null,null,null,null,null,null,"VERSION : 2.0"]
[]
[]
[]
[null,null,null,null,"ID","UNIQUE ID","Date Recorded","Type of Deficiency","Observer code","Type of Inspection","Description of Deficiency","Equipment Categories","Area of Observation","Deficiency Cause","VIQ Ref Number","Risk Value of Obs","PSC Ref Number","PSC MOU ID","Action Taken or Required","Target Date","PO Ref No.","Status Code","Date Completed","Drydock","Info Sharing","Critical Item","Audit Type","Superintendent Remarks"]
[null,null,null,null,2606,"57_21/10/2019 9:30:28 AM","2019-03-06","Defect","Ship Staff","Ship Staff Insp.","No.1 Main LO pump seal leak.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Pump seal has been renewed.","2019-06-05","","Completed","2019-03-18","No","No","No","Internal"]
[null,null,null,null,2592,"57_20/10/2019 00:23:33","2019-05-04","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Axe was missing from the axe box on upper deck.","LSA / FFA","Safety / LSA / FFA","Inappropriate Procedure","5.43","High","","","Same to be put back.","2019-05-11","","Completed","2019-05-07","No","No","No","Internal"]
[null,null,null,null,2593,"57_20/10/2019 00:31:27","2019-05-04","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Aft Mooring winch gear oil sight glass is dirty and hence, oil level is not visible.","Deck - Mooring Machinery","Mooring","Equipment Related","10.25","Very High","","","Same to be cleaned","2019-06-04","","Completed","2019-05-09","No","No","No","Internal"]
[null,null,null,null,2595,"57_20/10/2019 9:24:10 AM","2019-05-04","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Mooring wire are found dry and muddy in appereance.","Deck - Mooring Machinery","Mooring","Behaviour Based","9.17","High","","","To be cleaned and greased.","2019-06-04","","Completed","2019-05-17","No","No","No","Internal"]
[null,null,null,null,2596,"57_20/10/2019 9:28:22 AM","2019-05-04","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Vent for emergency DG room cofferdam, is not stencilled.","Miscellaneous","Eng. / Strg. Comp.","Behaviour Based","11.17","Low","","","proper stenciling to be done.","2019-05-14","","Completed","2019-05-13","No","No","No","Internal"]
[null,null,null,null,2597,"57_20/10/2019 9:33:09 AM","2019-05-04","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Stencil for fire sensor at various locations are not proper.  Same is written by permanent marker","Miscellaneous","Emgcy. Systems","Behaviour Based","5.4","High","","","Proper stenciling to be done","2019-05-14","","Completed","2019-05-13","No","No","No","Internal"]
[null,null,null,null,2607,"57_21/10/2019 9:37:06 AM","2019-05-04","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Poster for “Alkaline and acidic chemicals to be kept separate” is missing in chemical locker.","Documentation,Miscellaneous","Eng. / Strg. Comp.","Inappropriate Procedure","10.29","Medium","","","Poster prepared and posted","2019-05-11","","Completed","2019-05-10","No","No","No","External"]
[null,null,null,null,2611,"57_21/10/2019 10:02:27 AM","2019-05-04","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","There is no protection / curtains for Aft hydraulics power panel, even though sea water line is passing near the starter panel. In forward store starter panel, arrangement is made but in aft it is missing.","Miscellaneous","Eng. / Strg. Comp.","Inappropriate Procedure","10.37","Medium","","","Plastic curtain and rod fabricated and fitted in place.","2019-08-04","","Completed","2019-05-25","No","No","No","External"]
[null,null,null,null,5614,"57_23/10/2019 9:40:25 AM","2019-05-04","Defect","Ship Staff","Suptd. Insp.","ME LO Purifier temeprature is set at 88'c. temperature to be maintained at 95'C","E/R - Purifier","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","All engineers briefed about the same.And temperature maintained at 95'C","2019-05-05","","Completed","2019-05-05","No","No","No","Internal"]
[null,null,null,null,2594,"57_20/10/2019 00:43:56","2019-05-06","Defect","Ship Staff","Ship Staff Insp.","Aft hydraulic Mooring system, HP line flange in engine room(Boiler platform stbd side)  found having having leakage.","E/R - Pipes/ valves & fittings","Mooring","Equipment Related","10.29","Medium","","","HP pipe line O rings to be renewed and tested, no leakage.","2019-05-15","","Completed","2019-05-15","No","No","No","Internal"]
[null,null,null,null,2608,"57_21/10/2019 9:41:48 AM","2019-05-06","Defect","Ship Staff","Ship Staff Insp.","Aft hydraulic mooring system, HP line flange in engine room ( boiler platform stbd side) found having leakage.","Deck - Mooring Machinery","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","HP pipe flange O-rings renewed and tested, no leaks observed.","2019-05-15","","Completed","2019-05-15","No","No","No","Internal"]
[null,null,null,null,2610,"57_21/10/2019 9:53:21 AM","2019-05-15","Defect","Ship Staff","Ship Staff Insp.","FWG Sea water inlet thermomter faulty","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Thermometer renewed","2019-05-25","","Completed","2019-05-20","No","No","No","Internal"]
[null,null,null,null,2612,"57_21/10/2019 10:11:12 AM","2019-05-15","Defect","Ship Staff","Ship Staff Insp.","ME Fuel oil auto filter element discs poor condition/some damaged and needs to be renewed.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","The correct filter elements supplied and replaced. ","2019-07-30","DSTA 190005/190056","Completed","2019-07-04","No","No","No","Internal"]
[null,null,null,null,2616,"57_21/10/2019 10:28:25 AM","2019-06-30","Breakdown","Ship Staff","Ship Staff Insp.","# 2 AE Lub oil priming pump motor - winding zero insulation","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","New motor received at S'pore on 01st Sept'19. Fitted on 04th Sept and tested, working satisfactory.","2019-09-05","GC's143E,167E / RO -DSTA 190097","Completed","2019-09-04","No","No","No","Internal"]
[null,null,null,null,2613,"57_21/10/2019 10:14:40 AM","2019-07-16","Breakdown","Ship Staff","Ship Staff Insp.","ME # 7 Unit PMI sensor cable accidentally cut","E/R - Main Engine","Eng. / Strg. Comp.","Human Error","10.32","Very High","","","New complete sensor with cable and connector received at S'pore on 01 sept 19, fitted, checked, found normal reading. ","2019-09-15","RO -DSTA 190098","Completed","2019-09-02","No","No","No","Internal"]
[null,null,null,null,2614,"57_21/10/2019 10:18:48 AM","2019-07-16","Defect","Ship Staff","Ship Staff Insp.","IG Scrubber area - Oxygen sensor defective /calibration not possible.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","New sensor received at S'pore on 01st New sensor received at S'pore on 01st Sept'19, fitted , calibrated and sensor reading normal.","2019-09-15","RO -DSTA 190062","Completed","2019-09-02","No","No","No","Internal"]
[null,null,null,null,7394,"57_13/12/2019 7:06:11 PM","2019-08-02","Defect","Ship Staff","Ship Staff Insp.","Section 12 : Navigation lights and failure alarm not recorded during control test  in deck log book .\n\n\n\nWindow wiper are operational not recorded during control test  in deck log book .\n\n","Documentation","Navigation","Human Error","4.3","Medium","","","Same recorded in bridge note book. Refer to navigation procedures and navigation audit for entries to be made in bidge note book","2019-08-02","","Completed","2019-08-02","No","No","No","Internal"]
[null,null,null,null,7396,"57_13/12/2019 7:08:17 PM","2019-08-02","Defect","Ship Staff","Ship Staff Insp.","Section 13 : The following were not recorded in the Bridge Note Book:\n\n\n\n•\tVerify berth to berth passage plan is available\n\n•\tVerify Under Keel Clearance calculations have been completed correctly for the time of departure\n\n•\tCheck charts for intended voyage are updated and available and courses plotted berth to berth\n\n","Documentation","Navigation","Human Error","4.1","High","","","Same recorded in bridge note book. Vessel will refer bridge note book and navigation audit checklist to make correct entries in bridge note book","2019-08-02","","Completed","2019-08-02","No","No","No","Internal"]
[null,null,null,null,2618,"57_21/10/2019 10:38:42 AM","2019-08-15","Breakdown","Ship Staff","Ship Staff Insp.","ME #2 unit FO Distributor block and aft fuel valve HP pipe threads damaged.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","New FO Distributor block with HP pipe and spares received & renewed. ","2019-09-15","RO-DSTA 195037","Completed","2019-09-09","No","No","No","Internal"]
[null,null,null,null,7379,"57_13/12/2019 11:37:04 AM","2019-08-16","Defect","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","The current edition of IMO publication 'IAMSAR Manual Volume III,\n\n2019 Edition - Mobil Facilities' was not available on board. The vessel had an old edition of\n\nIAMSAR Manual Vol. III 2016 Edition, but it didn't include the relevant amendments addressed\n\nin the MSC.1/Circ.1594 effective from 1 July 2019. A dispatch order from the vendor, dated 18\n\nJuly 2019, confirmed this publication had been booked.","Navigation - Others","Navigation","Human Error","4.12","Very High","","","New Edition was received at Rizhao, China.","2019-08-31","","Completed","2019-08-23","No","No","No","External"]
[null,null,null,null,7380,"57_13/12/2019 11:40:31 AM","2019-08-16","Defect","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","There were two oxygen sensors installed in the space containing the\n\ninert gas system in the engine room. However, it was noted the oxygen sensor positioned near\n\nthe inert gas scrubber unit was malfunctioning. Vessel had carried out the risk assessment and\n\nadditional pre-caution measures were in place.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","8.3","Very High","","","New sensors were received at Singapore on 01st Sep 2019 & replaced.","2019-09-15","","Completed","2019-09-01","No","No","No","External"]
[null,null,null,null,7381,"57_13/12/2019 11:44:14 AM","2019-08-16","Defect","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","Evidence of master's feedback for STS operations carried out in March\n\nand July 2019 was not available on board.","Miscellaneous","Navigation","Human Error","8.54","High","","","Master's feedback was prepared & previous records updated.","2019-08-20","","Completed","2019-08-18","No","No","No","External"]
[null,null,null,null,2615,"57_21/10/2019 10:25:08 AM","2019-08-27","Breakdown","Ship Staff","Ship Staff Insp.","ME # 2 FO Circulating pump - drive screw sheared","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Spare screw kit received at S'pore. Pump boxed back with new spares on 02nd Sept and tested on 03rd Sept. Found working satisfactory. ","2019-09-05","RO-DSTA 195041","Completed","2019-09-03","No","No","No","Internal"]
[null,null,null,null,2587,"57_18/10/2019 22:33:23","2019-09-01","Breakdown","Ship Staff","Ship Staff Insp.","Port side bridge wing camera not working.","Navigation - Others","Navigation","Equipment Related","4.7","High","","","Camera received on 13th Jan 2020 after repairs from shore and fitted on 14th Jan 2020","2020-02-01","","Completed","2020-01-14","No","No","No","Internal","Repair is in progress. Will be connected next call Singapore."]
[null,null,null,null,2591,"57_20/10/2019 10:15:53 AM","2019-09-01","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Fire Station wakie talkie -one pouch missing (3 pouches for 4 walkie talkies)","LSA / FFA","Communication","Behaviour Based,Human Error","5.43","High","","","Missing Pouch returned in place.","2019-09-08","","Completed","2019-09-03","No","No","No","Internal"]
[null,null,null,null,2598,"57_20/10/2019 10:21:17 AM","2019-09-01","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Bosun Store-Instruction regarding fire extinguisher fallen on floor.","LSA / FFA","Safety / LSA / FFA","Behaviour Based","5.42","Medium","","","Instruction for fire extinguisher inside bosun store put back in place","2019-09-04","","Completed","2019-09-03","No","No","No","Internal"]
[null,null,null,null,2599,"57_20/10/2019 10:26:21 AM","2019-09-01","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Fire extinguisher at entrance to cargo pump room-not checked in Aug 2019","LSA / FFA","Safety / LSA / FFA","Behaviour Based","5.42","Medium","","","Fire extinguisher at the entrance of pump room Inspected.","2019-09-08","","Completed","2019-09-07","No","No","No","Internal"]
[null,null,null,null,2600,"57_20/10/2019 10:29:51 AM","2019-09-01","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Deck foam line valve in foam room(Valve 13)  leaking from gland.","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.38","High","","","Foam line Valve No 13 Gland packing tightening well and it is rectified.","2019-09-08","","Completed","2019-09-07","No","No","No","Internal"]
[null,null,null,null,2601,"57_20/10/2019 10:36:29 AM","2019-09-01","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Deck foam pump inlet and outlet line pressurised(beacause  of sea water flushing valve leaking(","Deck - Pipe / Fittings","Safety / LSA / FFA","Equipment Related","5.38","High","","","Flushing globe valve gland packing opened and lapping of surface carried.  Found holding good.","2019-09-19","","Completed","2019-09-19","No","No","No","Internal"]
[null,null,null,null,2602,"57_20/10/2019 1:41:51 PM","2019-09-01","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Stbd Windlass brg dry.  Greasing to be carried out.","Deck - Mooring Machinery","Mooring","Behaviour Based","9.2","Very High","","","Greasing carried out before heaving up anchor at Fujairah.","2019-09-20","","Completed","2019-09-20","No","No","No","Internal"]
[null,null,null,null,2603,"57_20/10/2019 1:45:51 PM","2019-09-01","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Mooring Choke on sunken deck not stencilled.","Deck - Mooring Machinery","Mooring","Behaviour Based","9.19","Low","","","Completed stenciling","2019-09-19","","Completed","2019-09-19","No","No","No","Internal"]
[null,null,null,null,2604,"57_20/10/2019 1:49:38 PM","2019-09-01","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Port Windlass Gear Oil look emulisified.  Gear Oil to be renewed.","Deck - Mooring Machinery","Mooring","Equipment Related","9.2","Very High","","","Port Windlass Gear Oil drained, cleaned inside chamber and renewed with new Oil.","2019-10-15","","Completed","2019-10-05","No","No","No","Internal"]
[null,null,null,null,2605,"57_20/10/2019 1:52:23 PM","2019-09-01","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Cargo Stripping Pump Gland Packing Leaking","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.18","High","","","Cargo Stripping Pump gland Packing renewed.","2019-10-08","","Completed","2019-10-05","No","No","No","Internal"]
[null,null,null,null,2609,"57_21/10/2019 9:47:21 AM","2019-09-01","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","In ECR AMS, communication error alarm existing for master clock interface","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","As per message and instructions from Kamlesh, ROS 2 computer was restarted and alarm was reset / master clock synchronized.","2019-09-30","","Completed","2019-09-29","No","No","No","External"]
[null,null,null,null,2617,"57_21/10/2019 10:33:44 AM","2019-09-01","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ER vent fan control panel showing inverter alarm","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","We have checked the inverter panel for the fans and had also tried to put off and on the power. As such there is no alarm on the inverter. The alarms seen on the remote (ECR) panel are of 2018 and don't know why they are showing. ","2019-09-11","","Completed","2019-09-10","No","No","No","External"]
[null,null,null,null,2619,"57_21/10/2019 10:44:36 AM","2019-09-01","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Steam leakage from overhead pipe aft of ME system oil storage tank","Deck - Pipe / Fittings,E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Gaskets renewed and leakage rectified. ","2019-10-01","","Completed","2019-09-14","No","No","No","External"]
[null,null,null,null,2620,"57_21/10/2019 10:48:22 AM","2019-09-01","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","SCR decomposition unit inlet thermometer faulty.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Thermometer renewed.","2019-09-30","","Completed","2019-09-21","No","No","No","External"]
[null,null,null,null,2621,"57_21/10/2019 10:52:00 AM","2019-09-01","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","220V low insulation- Insulation level at 2M ohm when deck lights are switched on.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","The low insulation was originating from the forward navigation light, same has been repaired and fault rectified. ","2019-09-30","","Completed","2019-09-27","No","No","No","External"]
[null,null,null,null,7382,"57_13/12/2019 1:32:07 PM","2019-09-01","Non Conformity","Owner / Marine / Tech. Suptd.","ISPS Audit","Gangway briefing for visitors was not done as per Goodwood best practice","Documentation","ISPS Related","Human Error","5.47","Medium","","","All crew briefed about the importance for safety and secuiry requirements  by keeping proper gangway watches.","2019-10-01","","Completed","2019-09-08","No","No","No","Internal"]
[null,null,null,null,7383,"57_13/12/2019 1:35:16 PM","2019-09-01","Non Conformity","Owner / Marine / Tech. Suptd.","ISM Audit","Ships ensign flag was not flown on the stern ","Miscellaneous","ISM Related","Human Error","","","","","All crewmembers briefed. Duty AB and Duty officer during take over to verify that the flags are properly deployed.","2019-10-01","","Completed","2019-09-08","No","No","No","Internal"]
[null,null,null,null,7384,"57_13/12/2019 1:38:12 PM","2019-09-01","Defect","Owner / Marine / Tech. Suptd.","ISM Audit","Life vest was not provided prior entry on the Billy Pug","Miscellaneous","ISM Related","Human Error","5.47","Medium","","","Life vest to  be kept tied on the personal transfer basket for immediate use. Crew briefing carried out, and duty officer  in charge and bosun to verify the same before lowering the basket.","2019-10-01","","Completed","2019-09-03","No","No","No","Internal"]
[null,null,null,null,7385,"57_13/12/2019 1:41:44 PM","2019-09-01","Defect","Owner / Marine / Tech. Suptd.","ISM Audit","Gangway placard - no smart watches permitted - is not stenciled","Miscellaneous","ISM Related","Inappropriate Procedure","5.47","Medium","","","All required information to be stenciled on the notice board, as per HSQEEn requiremnt. Crew briefed about the safety requirement needed on deck , and the consequence of a hazard if using smart watches on deck.  Any information required to be displayed should be stenciled as soon as possible with out delay.","2019-10-01","","Completed","2019-09-07","No","No","No","Internal"]
[null,null,null,null,7386,"57_13/12/2019 1:50:20 PM","2019-09-01","Non Conformity","Owner / Marine / Tech. Suptd.","ISM Audit","2 scuppers (stbd aft main deck) & i.w.o. 3 (S) COT were found un-shipped during bunker operations ","Hull & Tanks","MARPOL Related","Human Error","6.2","High","","","Scuppers to be plugged well before arrival, port and only the aft 2 scuppers to be left open for rain water to drain before arrival.  As crew will be busy after arrival port, this will save time. Duty officers to verify, and at least  2 persons to visually  to confirm and report that the scuppers are in place.","2019-10-01","","Completed","2019-09-08","No","No","No","Internal"]
[null,null,null,null,7387,"57_13/12/2019 1:53:14 PM","2019-09-01","Non Conformity","Owner / Marine / Tech. Suptd.","ISM Audit","Vessel equipped with fixed piping to manage oil spills on main deck. But fuel tank air pipes are located aft main deck - with no facilities to contain a spill ","Miscellaneous","MARPOL Related","Human Error","6.3","Low","","","During bunkering time, seperate portable wilden pump to be rigged aft of the fish plate to tackle , spillls from bunker tank vents. Duty officer and person incharge of the operation to verify portable wilden pump is rigged before the bunkering starts.","2019-10-01","","Completed","2019-09-08","No","No","No","Internal"]
[null,null,null,null,7388,"57_13/12/2019 5:45:13 PM","2019-09-01","Defect","Owner / Marine / Tech. Suptd.","ISM Audit","Minor Hydraulic leak was sighted forward of P/R entrance ","Cargo Mach.","Cargo / Ballast Systems","External Factors","6.3","Low","","","Any leakages on deck to be rectified as soon as possible, and the area to be cleaned prior arrival port.Leakages to be checked and ientified during the safety rounds and repairs to be carried out as soon as possible before arrival port.","2019-10-01","","Completed","2019-09-09","No","No","No","Internal"]
[null,null,null,null,7389,"57_13/12/2019 5:49:24 PM","2019-09-01","Defect","Owner / Marine / Tech. Suptd.","ISM Audit","Port anchor hawse pipe - cover was not firmly fixed. It was easily opened with just one tug as the locking pins were not secured ","Hull & Tanks","General Appearance","Human Error","7.12","High","","","Crew and officers briefed, and the requirement of closing the anchor hawse pipe to prevent robbery discussed. After dropping anchor each time, crew to cover the anchor hawse pipe cover properly and Chief officer to verfiy and report. ","2019-10-01","","Completed","2019-09-09","No","No","No","Internal"]
[null,null,null,null,7390,"57_13/12/2019 6:51:00 PM","2019-09-01","Non Conformity","Owner / Marine / Tech. Suptd.","Engineering Audit","In ECR - alarm monitoring system - MSBD abnormal alarm found off scan ","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Knowledge Based","10.2","Low","","","MSBD alarm offscan disabled and all engineers briefed on the consequences.All engineers were briefed about importances of certain alarms and consequences in offscanning of alarms. Without chief engineer permission no alarms to be offscanned or disabled. ","2019-10-01","","Completed","2019-09-01","No","No","No","Internal"]
[null,null,null,null,5599,"57_23/10/2019 9:55:21 AM","2019-09-01","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","LO drums were lifted without using safety lead to control swing. Crew to be briefed\t\t","Miscellaneous","Crew Management","Human Error,Inappropriate Procedure","5.11","Low","","","All crew briefed during toolbox meeting after  departure port","2019-09-08","","Completed","2019-09-04","No","No","No","Internal"]
[null,null,null,null,7391,"57_13/12/2019 6:54:36 PM","2019-09-01","Defect","Owner / Marine / Tech. Suptd.","ISM Audit","LO drums were lifted without using safety lead to control swing","Miscellaneous","Crew Management","Human Error","","","","","Crew to be tie at least two lead line to prevent the swing on the drum  And thus preventing the wild swing. Crew briefed and trained, specially for these jobs. Supervision of the job  by officer incharge, and immedeate stop work procedure incase of any wrong action.","2019-10-01","","Completed","2019-09-03","No","No","No","Internal"]
[null,null,null,null,5600,"57_23/10/2019 9:58:29 AM","2019-09-01","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Small steels pipes in ER workshop not lashed\t","Miscellaneous","Eng. / Strg. Comp.","Behaviour Based,Inappropriate Procedure","5.11","Low","","","small steel pipes etc removed ,placed properly and lashed.","2019-09-04","","Completed","2019-09-03","No","No","No","Internal"]
[null,null,null,null,5601,"57_23/10/2019 10:02:42 AM","2019-09-01","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Grey water pump leaking from flange\t","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","gasket changed, save all trays painted","2019-09-08","","Completed","2019-09-07","No","No","No","Internal"]
[null,null,null,null,7393,"57_13/12/2019 7:02:04 PM","2019-09-01","Defect","Owner / Marine / Tech. Suptd.","Nav Audit / Verification","Masters's signature on flwg were not available from 21 Aug. Deck log book, Bell book , GMDSS log books\n\n","Documentation","Cert. & Docu.","Human Error","4.23","High","","","All officers briefed, regarding the strict requirement of keeping bridge watches and handing over requirement.All officers to complete their log book and sign and relieving officer to check, and report to master.  Master  & chief officer to check and verify  and complete log books for the previous day .","2019-11-01","","Completed","2019-09-16","No","No","No","Internal"]
[null,null,null,null,5602,"57_23/10/2019 10:38:44 AM","2019-09-01","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","IG system fresh air intake flange wing nuts to ease up\t","Inert Gas","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Wing nuts eased up and greased","2019-09-08","","Completed","2019-09-08","No","No","No","Internal"]
[null,null,null,null,5603,"57_23/10/2019 10:42:18 AM","2019-09-01","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp."," MGO filling line safety valve opening pressure not stencilled\t\t\t\t\t\t\t\t","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Behaviour Based,Equipment Related","10.8","Medium","","","opening pressure stencilled- 5.0bar","2019-09-08","","Completed","2019-09-03","No","No","No","Internal"]
[null,null,null,null,5604,"57_23/10/2019 10:45:07 AM","2019-09-01","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Lifting hooks in steering gear room\t","Miscellaneous","Eng. / Strg. Comp.","Inappropriate Procedure","10.28","Low","","","all hooks color coded and SWL color code laminated poster posted in steering gear room","2019-09-18","","Completed","2019-09-18","No","No","No","Internal"]
[null,null,null,null,5605,"57_23/10/2019 11:34:13 AM","2019-09-01","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Main engine attached hydraulic pump no:3 accumulator cap has fallen down\t","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Cap fitted back","2019-09-30","","Completed","2019-09-25","No","No","No","Internal"]
[null,null,null,null,5606,"57_23/10/2019 11:37:34 AM","2019-09-01","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Rudder rams (P fwd & Aft) have more leakage than stbd ones\t","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Packing gland tightened as per maker instructions, oil leak reduced, under observation","2019-10-01","","Completed","2019-09-25","No","No","No","Internal"]
[null,null,null,null,5607,"57_23/10/2019 11:40:32 AM","2019-09-01","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","In ECR ams, communication error alarm existing for master clock interface\t\t","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","As per msg from Suptd. Kamlesh, ROS2 computer restarted annd alarm was reset. Master clock interface working in order.","2019-09-30","","Completed","2019-10-01","No","No","No","Internal"]
[null,null,null,null,5608,"57_23/10/2019 11:43:39 AM","2019-09-01","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Spare hydraulic motors for windlass and winch kept in steering gear room to identify and also update in PAL PMS\t","Miscellaneous","Eng. / Strg. Comp.","Behaviour Based","5.11","Low","","","Spare motors shifed to mid ship locker and location in PAL updated","2019-10-01","","Completed","2019-10-14","No","No","No","Internal"]
[null,null,null,null,5615,"57_23/10/2019 9:46:54 AM","2019-09-01","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","In ECR Alarm monitoring system \"MSBD abnormal\" alarm found offscan\t\t\t\t","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Behaviour Based,Equipment Related","10.38","Medium","","","Removed from offscan, alarm reset","2019-09-02","","Completed","2019-09-01","No","No","No","Internal"]
[null,null,null,null,5616,"57_23/10/2019 11:46:19 AM","2019-09-01","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","C2E feed pump discharge pressure guage needle broken\t","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.31","Very High","","","pressure guage renewed with spare","2019-10-08","","Completed","2019-10-15","No","No","No","Internal"]
[null,null,null,null,7392,"57_13/12/2019 6:58:23 PM","2019-09-05","Defect","Ship Staff","Ship Staff Insp.","Poor quality Squid supplied by ship chandellor ","Accommodation","MLC Related","External Factors","","","","","If bad quality items supplied, immedeately return back the items, and report the matter to company.Prior instructions to be given, to ship chandler, that if any  items are found ito be in a bad condition, it will be rejected and  returned by the same boat.","2019-09-20","","Completed","2019-09-15","No","No","No","Internal"]
[null,null,null,null,2588,"57_20/10/2019 4:51:03 PM","2019-09-12","Defect","Ship Staff","Ship Staff Insp.","BWTS No 1 Loop Filter inlet valve BA 614 & No1 loop filter Bypass valve BA 616 suspect valve passing in closed position.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","6.21","High","","","Both Vaves were observed for integrity during ballasting operation at PAL, USWC and confimred to be holding. Will monitor again during Ballast exchange prior arrival Loadport.","2019-12-11","","Completed","2019-11-09","No","No","No","Internal","Vessel is supplied with spare seat rings for ballast line. Renew seat rings if valves are leaking."]
[null,null,null,null,2590,"57_18/10/2019 22:47:02","2019-09-12","Defect","Ship Staff","Ship Staff Insp.","Ballast valves BA508 & BA510 is kept at 20% open to prevent the valve to be stuck at closed position.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.11","Medium","","","Both the valves renewed & tested. Working satisfactorily.","2019-12-11","DSTA-190089","Completed","2019-10-13","No","No","No","Internal"]
[null,null,null,null,7400,"57_13/12/2019 12:58:05 PM","2019-11-06","Defect","Owner / Marine / Tech. Suptd.","Nav Audit / Verification","Echo sounder scale in Use not mentioned for Departure Rastanura on 26th Sept 2019.","Documentation","Navigation","Human Error","4.19","Low","","","Appropriate entries made & observation has been closed out.","2020-02-06","","Completed","2019-11-12","No","No","No","Internal"]
[null,null,null,null,7401,"57_13/12/2019 1:03:06 PM","2019-11-06","Defect","Owner / Marine / Tech. Suptd.","Nav Audit / Verification","Company Standing Orders and Master's Standing Orders not countersigned by Watch keeping Ratings.","Documentation","Navigation","Human Error","4.1","High","","","Ratings were briefed regarding the requirement. Master's & Company Standing orders were countersigned by Watch ratings & observation closed out. ","2020-02-06","","Completed","2019-11-13","No","No","No","Internal"]
[null,null,null,null,7402,"57_13/12/2019 1:05:58 PM","2019-11-06","Defect","Owner / Marine / Tech. Suptd.","ISPS Audit","Gangway log not properly filled up for Visitor card numbers at Rastanura.","Documentation","ISPS Related","Human Error","7.12","High","","","Approrpiate entries were made & observation closed out. Crew briefing carried out to prevent recurrence.","2020-02-06","","Completed","2019-11-15","No","No","No","Internal"]
[null,null,null,null,7403,"57_13/12/2019 1:14:45 PM","2019-11-06","Defect","Owner / Marine / Tech. Suptd.","ISM Audit","Cargo tank valve operation log for loading at Rastanura not completed.","Documentation","Cargo / Ballast Systems","Human Error","8.12","Medium","","","Cargo tank valve operation log was completed. Officers were given training to prevent recurrence.","2020-02-06","","Completed","2019-11-13","No","No","No","Internal"]
[null,null,null,null,7404,"57_13/12/2019 1:16:33 PM","2019-11-06","Non Conformity","Owner / Marine / Tech. Suptd.","ISM Audit","Toolbox meeting section for “Days jobs completed to Satisfaction and Verified by” not signed by Concerned officer from 15th Oct 2019 to 01st Nov 2019","Documentation","ISM Related","Human Error","5.2","Very High","","","Required entries made & NC closed out. Training conducted to prevent recurrence.","2020-02-06","","Completed","2019-11-20","No","No","No","Internal"]
[null,null,null,null,7405,"57_13/12/2019 1:25:14 PM","2019-11-06","Defect","Owner / Marine / Tech. Suptd.","ISM Audit","Vessel was carrying High H2S Cargo however “Precautions when carrying High H2S Cargoes” was not posted in Common spaces of Accommodation.","Documentation","ISM Related","Human Error","5.47","Medium","","","Required Poster prepared and put up at Various locations.","2020-02-06","","Completed","2019-11-14","No","No","No","Internal"]
[null,null,null,null,7406,"57_13/12/2019 1:08:09 PM","2019-11-06","Defect","Owner / Marine / Tech. Suptd.","MLC Audit","Knives used for cutting Meat and Vegetables are not Color coded as per the Color code chart in the Galley.","Accommodation","MLC Related","Knowledge Based","11.13","Low","","","Color coding done for various knives and observation closed out.","2020-02-06","","Completed","2019-11-15","No","No","No","Internal"]
[null,null,null,null,7407,"57_13/12/2019 1:18:41 PM","2019-11-06","Defect","Owner / Marine / Tech. Suptd.","ISM Audit","Flame screen of 2S P/V Valve (Vacuum side) dislodged from the frame on one side.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.19","High","","","Dislodged section of Flame Screen fitted back in position & observation closed out.  ","2020-02-06","","Completed","2019-11-16","No","No","No","Internal"]
[null,null,null,null,7408,"57_13/12/2019 1:11:39 PM","2019-11-06","Defect","Owner / Marine / Tech. Suptd.","Engineering Audit","Scope of Implementation starting date for 10) Propeller maintenance (Cleaning / Polishing) not mentioned in the Action Plan","Documentation","Cert. & Docu.","Inappropriate Procedure","10.12","Very High","","","Action plan amended and observation closed out.","2020-02-06","","Completed","2019-11-12","No","No","No","Internal"]
[null,null,null,null,7409,"57_13/12/2019 1:22:26 PM","2019-11-06","Defect","Owner / Marine / Tech. Suptd.","ISM Audit","No locking or sealing arrangement is provided for Galley comminutor.","Accommodation","MARPOL Related","Inappropriate Procedure","6.2","High","",""," locking arrangement made, poster pasted near the commuter. also breaker will be kept off in port.","2020-02-06","","Completed","2020-01-06","No","No","No","Internal"]
[null,null,null,null,5610,"57_23/10/2019 11:48:48 AM","2019-11-08","Breakdown,Defect","Ship Staff","Ship Staff Insp.","Steering gear rudder carrier greasing pump body cracked","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Spares received at singapore on 13/01/2020. New grease pump fitted, working staisfactory.","2020-02-12","DSTA190159","Completed","2020-01-25","No","No","No","Internal","Spare is ready for supply. Waiting for convenient port. Revise target date as spare can be supplied at Singapore only."]
[null,null,null,null,6285,"57_20/11/2019 2:33:15 PM","2019-11-12","Breakdown","Ship Staff","Ship Staff Insp.","Experiencing issues with Bridge Window Wiper controller panel. At present, the following wipers are in-operational :\n\nWiper No.1 \n\nWiper No.3 \n\nWiper No.5\n\nWiper No.6\n\nWiper No.7\n\nWiper No.9","Navigation - Others","Navigation","Equipment Related","4.7","High","","","New controller panel and senser received and fitted. system working satisfactory","2020-02-11","DSTA190174","Completed","2020-01-15","No","No","No","Internal","Spare will be ready on 10th Jan. Will be connected accordingly."]
[null,null,null,null,6286,"57_20/11/2019 11:06:06 PM","2019-11-12","Other","Owner / Marine / Tech. Suptd.","Ship Staff Insp.","Job operational spares to be updated in PAL.","Miscellaneous","Cert. & Docu.","Inappropriate Procedure","","","","","Job Operational spares to be updated in PAL.","2020-01-25","","Completed","2020-01-10","No","No","No","Internal","Complete this job ASAP."]
[null,null,null,null,7395,"57_13/12/2019 7:19:23 PM","2019-11-19","Defect","Owner / Marine / Tech. Suptd.","ISM Audit","12.20.05.011.04 Pre Arrival and commencement of cargo Operation checklist for loading at Juaymah - Section B (To be completed 24 Hrs prior operation) completed on 21 Sept 2019 at 1500 LT while loading operation commenced on 24 Sept 2019 1325 Hrs. ","Documentation","Cargo / Ballast Systems","Human Error","2.3","High","","","Required entries made & observation has been closed out.","2019-12-19","","Completed","2019-12-02","No","No","No","Internal"]
[null,null,null,null,7397,"57_13/12/2019 7:29:03 PM","2019-11-19","Defect","Owner / Marine / Tech. Suptd.","ISM Audit","CCR Movement Log : Entry for Independent check of Line up did not include Venting prior Loading operation at Juaymah on 24 Sept 2019.","Documentation","ISM Related","Human Error","2.3","High","","","Required entries made & observation has been closed out.","2019-12-19","","Completed","2019-12-02","No","No","No","Internal"]
[null,null,null,null,7398,"57_13/12/2019 7:31:23 PM","2019-11-19","Defect","Owner / Marine / Tech. Suptd.","ISM Audit","Pre Arrival Tests and Checks prior Loading at Juaymah did not include any test and checks for BWTS system.","Documentation","ISM Related","Human Error","2.3","High","","","Required entries made & observation has been closed out.","2019-12-19","","Completed","2019-12-02","No","No","No","Internal"]
[null,null,null,null,7399,"57_13/12/2019 7:34:04 PM","2019-11-19","Defect","Owner / Marine / Tech. Suptd.","Bunkering Audit","Bunker Transfer Plan / Checklist 12.04.08.011.01 Section 7 - Monitoring of H2S/Benzene Vapors : \n\nBenzene reading measured by detector tubes shall be mentioned < Min value that can be measured by the specific tube. For example by Gastec tubes Min measurable value is 0.05 ppm, hence in that case benzene shall be mention <0.05 ppm (if no discoloration observed)\n\nUnderstand vessel has kept the Gas tubes as evidence of monitoring.\n\n","Documentation","ISM Related","Human Error","10.8","Medium","","","Required entires made & observation has been closed out.","2019-12-19","","Completed","2019-12-02","No","No","No","Internal"]
[null,null,null,null,5609,"57_22/10/2019 2:23:29 PM","2019-11-22","Defect","Ship Staff","Ship Staff Insp.","Cargo Oil tank Pressure Sensor for 1 Port tank and 4 Stbd Showing erratic","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.13","Medium","","","1P Pressure sensor renewed with spare sensor available onboard and is presently under observation.                                                           Cargo tank Pressure sensor for 4S renewed with new spare. working satisfactory.","2020-02-21","DSTA190156","Completed","2020-01-21","No","No","No","Internal","3 nos, spare sensors are on order, for vessel to keep 1 as spare. Will be connected next call Singapore."]
[null,null,null,null,5611,"57_27/10/2019 8:15:30 AM","2019-11-24","Defect","Ship Staff","Ship Staff Insp.","Red warning  light Glass  Shade for Hose handling crane Port side broken","Deck - Machinery,Elect. Mach. & Equip.","Emgcy. Systems","Equipment Related","8.63","High","","","Complete new fitting with glass receive at singapore on 13/01/2020. Working satisfactory.","2020-02-23","DSTA-190163","Completed","2020-01-21","No","No","No","Internal","Liaise with procure - give details of spare required and maker."]
[null,null,null,null,6284,"57_Fri Jan 11 2019 05:50:52 GMT+0000 (Coordinated Universal Time)","2019-11-30","Breakdown,Defect","Ship Staff","Ship Staff Insp.","Fwd Anchor light and fitting damaged","Navigation - Others","Navigation","Equipment Related,External Factors","4.8","Medium","","","Fwd Anchor light fitting replaced and tried satisfactorily ","2020-03-31","DSTA190166","Completed","2020-03-10","No","No","No","Internal"]
[null,null,null,null,7410,"57_15/12/2019 10:19:36 AM","2019-12-18","Defect","Ship Staff","Ship Staff Insp.","Navigation light failure alarm for Port Main Side light is in-operative.","Navigation - Others","Navigation","Equipment Related","4.3","Medium","","","Navigation Alarm PCB replaced and alarm tried out satisfactorily ","2020-03-31","DSTA-190157","Completed","2020-03-10","No","No","No","Internal","Spare will be ready by 1st Jan 2020. Will be connected while passing Singapore."]
[null,null,null,null,9054,"57_26/12/2019 4:31:04 AM","2019-12-21","Defect","Ship Staff","Ship Staff Insp.","DG Viscotherm showing wrong values","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.1","Medium","","","Sensor received and replaced, working - satisfactory","2020-01-31","Spare requested on excel sheet","Completed","2020-01-20","No","No","No","Internal","PO under process. Getting quotation from various suppliers."]
[null,null,null,null,9868,"57_11/1/2020 7:09:25 AM","2020-01-02","Defect","Ship Staff","Ship Staff Insp.","BWTS c2e unit flow meter 952 is defective.","E/R - Aux. Mach.","Cargo / Ballast Systems","Equipment Related","6.22","Medium","","","Fow meter 952 found choked with salt deposits. cleaned and tried out found working satisfactory","2020-03-31","DSTA200009","Completed","2020-03-31","No","No","No","Internal"]
[null,null,null,null,9869,"57_11/1/2020 7:33:22 AM","2020-01-05","Defect","Ship Staff","Ship Staff Insp.","Engine room store packeged A/C pressure switch is defective.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.1","Medium","","","pressure switch replaced with new one.","2020-02-28","DSTA200017","Completed","2020-02-05","No","No","No","Internal"]
[null,null,null,null,10405,"57_28/1/2020 10:50:54 AM","2020-01-19","Defect","Ship Staff","Ship Staff Insp.","ME unit no.7 second piston ring broken at butt area(app.40mm)","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.1","Medium","","","ME unit#7 all piston rings renewed by service engineer with shore staff.","2020-02-28","","Completed","2020-02-02","No","No","No","Internal"]
[null,null,null,null,10451,"57_Wed Feb 12 2020 10:29:02 GMT+0000","2020-02-02","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Temperature log sheet for CO2 cylinder for Emergency DG room missing.","LSA / FFA","Safety / LSA / FFA","Inappropriate Procedure","5.35","Medium","","","temperature log sheet put in place and updated on weekly basis.","2020-02-28","","Completed","2020-02-05","No","No","No","Internal"]
[null,null,null,null,10452,"57_Wed Feb 12 2020 10:33:55 GMT+0000","2020-02-02","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Quick closing valve for emergency DG operating box rusted.","LSA / FFA","General Appearance","Equipment Related","10.17","Very High","","","Box derusted and painted.","2020-02-29","","Completed","2020-02-05","No","No","No","Internal"]
[null,null,null,null,10453,"57_Wed Feb 12 2020 10:46:57 GMT+0000","2020-02-02","Non Conformity","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Restricted area not tagged. Tags not found in emergency DG room, CO2 room and various other restricted area.","LSA / FFA","ISPS Related","Inappropriate Procedure","7.5","Low","","","All restricted area  identified and tagged.","2020-02-29","","Completed","2020-02-06","No","No","No","Internal"]
[null,null,null,null,10454,"57_Wed Feb 12 2020 11:05:14 GMT+0000","2020-02-02","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Various dampers in ME exhaust line to grease","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Greasing carried out as per lube oil chart, renolit lx-pep 2/3.","2020-03-31","","Completed","2020-02-16","No","No","No","Internal"]
[null,null,null,null,10455,"57_Wed Feb 12 2020 11:23:19 GMT+0000","2020-02-02","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Engine room vent fan control panel in alarm condition.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Spare cooling fans received renewed for ER supply fan no 1 and 4. Now working satisfactory and no alarm indication is present. Job order no: V-DSTA020980/21, V-DSTA020979/21","2021-02-28","","Completed","2021-01-29","No","No","No","Internal","Spare is ready for supply."]
[null,null,null,null,10475,"57_Sat Feb 15 2020 09:27:07 GMT+0000","2020-02-02","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Main Engine LO purifier operating at 81 deg C","E/R - Purifier","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","LO purifier temperature increased to 94 degree and same instructed to ship staff.","2020-02-20","","Completed","2020-02-02","No","No","No","Internal"]
[null,null,null,null,10476,"57_Sat Feb 15 2020 09:30:58 GMT+0000","2020-02-02","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Sewage Treatment Plant re-circulation flow not visible.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","transparent pipe replaced with new one, line cleared. now flow is clearly visible.","2020-02-29","","Completed","2020-02-06","No","No","No","Internal"]
[null,null,null,null,10477,"57_Sat Feb 15 2020 09:34:01 GMT+0000","2020-02-02","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","220V insulation at 10 M ohm.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.38","Medium","","","low insulation was coming from service air dryer drain solenoid valve same rectified.","2020-02-29","","Completed","2020-02-10","No","No","No","Internal"]
[null,null,null,null,10478,"57_Sat Feb 15 2020 09:37:19 GMT+0000","2020-02-02","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","3C, 4S, 3S cargo tank dome packing to renew.","Hull & Tanks","Cargo / Ballast Systems","Equipment Related","2.16","Medium","","","All butterfly nuts were unevenly tightened; currently no leaks after nuts were evenly tightened","2020-03-31","","Completed","2020-02-08","No","No","No","Internal"]
[null,null,null,null,10479,"57_Sat Feb 15 2020 09:42:44 GMT+0000","2020-02-02","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Windlass stbd and port gear oil emulsified.","Deck - Mooring Machinery","Mooring","Equipment Related","9.2","Very High","","","Gear oil renewed in WI (Stbd windlass). W2 (Port windlass) oil found in good condition","2020-03-31","","Completed","2020-04-07","No","No","No","Internal"]
[null,null,null,null,10480,"57_Sat Feb 15 2020 09:44:39 GMT+0000","2020-02-02","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Brake clearance to check and adjust for all Winches and Windlass.","Deck - Mooring Machinery","Mooring","Equipment Related","9.15","Medium","","","All Winches Brake Adjustment check nuts adjusted and freed as required ","2020-03-31","","Completed","2020-03-07","No","No","No","Internal"]
[null,null,null,null,11438,"57_27/3/2020 11:49:36 PM","2020-03-27","Observation","Ship Staff","Ship Staff Insp.","Main engine Unit #6 piston rings found having scuffing and middle piston ring found broken at the end","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","ME Unit #6 Piston rings renewed with cermet coated rings , Cylinder liner renewed by shore team. Investigation carried out by MAN technician, HSD and ship staff for the scuffing.Corrective and preventive actions taken as advised.","2020-04-05","","Completed","2020-04-05","No","No","No","Internal"]
[null,null,null,null,11437,"57_16/4/2020 2:42:42 PM","2020-04-06","Critical Equipment","Ship Staff","Ship Staff Insp.","Cargo OB discharge v/v CL-151 (solenoid fitting in R/Rm) has to be manually moved once command (for OPEN/SHUT) given by the ODME panel","Critical Equip.","Eng. / Strg. Comp.","Equipment Related","6.13","Low","","","New Flowmeter with Open/Shut limit switch requistioned - awaiting spares. Time being the system can be operated but one person needs to stby at the solenoid box while ODME is tested/operational","2020-07-31","DSTA200099","Completed","2020-07-09","No","No","No","Internal","Spare will be supplied at Singapore on 2nd July."]
[null,null,null,null,11608,"57_30/4/2020 4:01:13 AM","2020-04-20","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","BWTS SYSTEM- Minor leak from anolyte pump","E/R - Pumps","Cargo / Ballast Systems","Equipment Related","10.29","Medium","","","Leak rectified","2020-10-31","","Completed","2020-09-03","No","No","No","Internal","Please mention RO no or  GC no . Target date revised."]
[null,null,null,null,11609,"57_30/4/2020 2:35:43 AM","2020-04-20","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Cold repair on STBD life boat cooling water tank","LSA / FFA","Emgcy. Systems","Equipment Related","10.31","Very High","","","The cracked/ damaged exhaust manifold pipe replaced with spare new one. Engine tried out staisfactory.","2021-02-28","","Completed","2021-01-28","No","No","No","Internal","Spare is ready at Singapore. Will be supplied while passing Singapore."]
[null,null,null,null,11610,"57_30/4/2020 4:45:36 AM","2020-04-20","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","No.1 Main LO pump- Lip seal leaking","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Seal renewed , same found leaking again. JOB PENDING. Seal leak checked in port and found very slight oil leaks when pump is in operation need seal sleeve renewal","2021-03-31","DSTA200084","Completed","2020-06-19","No","No","No","Internal","Check LO return pipe as advised by maker."]
[null,null,null,null,11611,"57_30/4/2020 10:14:52 PM","2020-04-20","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Out of 32 COT hatches - Rubber packing for 19 were renewed due to leaks. Remaining 13 COT hatches not leaking but suggest to change at 1st oppurtunity","Hull & Tanks","Cargo / Ballast Systems","Equipment Related","8.21","High","","","Spares received,renewal of leaking cargo tankdome rubber packing completed","2020-10-31","DSTA200111","Completed","2020-08-25","No","No","No","Internal","Job in progress. Target date revised."]
[null,null,null,null,11612,"57_23/4/2020 11:53:21 PM","2020-04-20","Critical Equipment","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ODME  ovbd valve  CL151 valve block indicator not working","Critical Equip.","Cargo / Ballast Systems","Equipment Related","","","","","Defective spare part to be renewed.","2020-08-18","","Completed","2020-07-09","No","No","No","Internal"]
[null,null,null,null,11613,"57_30/4/2020 10:24:38 PM","2020-04-20","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Pipes fretting due to vibration","Deck - Pipe / Fittings","Cargo / Ballast Systems","Industry Issue","","","","","Teflon padding to put to prevent fretting damage to pipes at two locations","2020-10-31","","Completed","2020-09-15","No","No","No","Internal","When expected to complete?"]
[null,null,null,null,11614,"57_23/4/2020 11:33:34 PM","2020-04-20","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Engine bell book recording not as per check list 12.01.10.021.00","Documentation","Cert. & Docu.","Human Error","10.5","Low","","","Follow instruction strictly as per 12.01.10.021.00. Record starting/stopping additional DG etc","2020-05-05","","Completed","2020-04-20","No","No","No","Internal"]
[null,null,null,null,11615,"57_24/4/2020 12:03:49 AM","2020-04-20","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","CE night order book -Last entry was 11 March. No instruction found for last cargo discharge/arrival/dep discharge port etc","Miscellaneous","Cert. & Docu.","Behaviour Based,Human Error","10.5","Low","","","Started writing night order book regularly to comply with VIQ requirements","2020-05-05","","Completed","2020-04-20","No","No","No","Internal"]
[null,null,null,null,11616,"57_30/4/2020 2:42:07 AM","2020-04-20","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","CO2 System for Emcy Gen Room- CO2 bottles found rusted at bottom","LSA / FFA","Emgcy. Systems","Equipment Related","10.1","Medium","","","CO2 bottles derusted and painted after obtaining critical work permit. ","2020-05-20","","Completed","2020-04-27","No","No","No","Internal"]
[null,null,null,null,11617,"57_30/4/2020 2:50:17 AM","2020-04-20","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Emergency DG Radiator air inlet duct damper solenoid valve-air leak","Critical Equip.","Emgcy. Systems","Equipment Related","10.1","Medium","","","Solenoid valve of emcy DG overhauled and rectified the leak. System operation tried out-found working satisfactory","2020-05-20","","Completed","2020-04-20","No","No","No","Internal"]
[null,null,null,null,11618,"57_30/4/2020 2:45:27 AM","2020-04-20","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Emergency DG -Manual starting mode lamp not working","Elect. Mach. & Equip.","Emgcy. Systems","Equipment Related","10.1","Medium","","","Renewed the defective indication lamp","2020-05-05","","Completed","2020-04-20","No","No","No","Internal"]
[null,null,null,null,11619,"57_30/4/2020 2:59:44 AM","2020-04-20","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Garbage drums near incinerator loosely lashed","Miscellaneous","General Appearance","Equipment Related","10.1","Medium","","","Garbage drums wire lashing made tight","2020-04-30","","Completed","2020-04-25","No","No","No","Internal"]
[null,null,null,null,11620,"57_30/4/2020 3:03:25 AM","2020-04-20","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","O2 sensor near IG area showing O2 % 22","Miscellaneous","Safety / LSA / FFA","Equipment Related","10.1","Medium","","","O2 sensor calibrated. Now showing O2 -20.9 %","2020-05-05","","Completed","2020-05-20","No","No","No","Internal"]
[null,null,null,null,11621,"57_30/4/2020 3:12:40 AM","2020-04-20","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ME exhaust line dampers to be greased","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.1","Medium","","","All dampers greased.","2020-04-30","","Completed","2020-04-20","No","No","No","Internal"]
[null,null,null,null,11622,"57_23/4/2020 11:45:23 PM","2020-04-20","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Air cooler drain line modified","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.1","Medium","","","Drain connection put back to  normal.Hole made on the manhole cover welded with insert plate","2020-05-05","","Completed","2020-04-25","No","No","No","Internal"]
[null,null,null,null,11623,"57_30/4/2020 4:11:40 AM","2020-04-20","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","FWD/AFT HPU Cooler- Cavitation noise observed from","Deck - Machinery","Eng. / Strg. Comp.","Equipment Related","10.39","High","","","Routine practice for shutting cooler inlet valve already in practice.","2020-04-30","","Completed","2020-04-20","No","No","No","Internal"]
[null,null,null,null,11624,"57_30/4/2020 4:29:39 AM","2020-04-20","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Steam leak above ICO lube","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Steam line flange retightened- rectified steam leak","2020-04-30","","Completed","2020-04-20","No","No","No","Internal"]
[null,null,null,null,11625,"57_30/4/2020 4:41:38 AM","2020-04-20","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Cargo pumps and Ballast pumps- Bulkhead seal grease pot level below red mark","E/R - Aux. Mach.","Cargo / Ballast Systems","Equipment Related","10.1","Medium","","","Topped up grease to the red mark wherever level found below red mark.","2020-05-05","","Completed","2020-04-20","No","No","No","Internal"]
[null,null,null,null,11626,"57_30/4/2020 3:45:47 PM","2020-04-20","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Emergency fire pump room drain cock frozen","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.1","Medium","","","Drain cock overhauled - well lubricated and eased up- working satisfactorily.","2020-05-20","","Completed","2020-04-20","No","No","No","Internal"]
[null,null,null,null,11627,"57_23/4/2020 11:57:42 PM","2020-04-20","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","main switch board -220 V low insulation","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.24","Low","","","Traced out earth fault and rectified . Now reading b/w 10 and infinity","2020-05-05","","Completed","2020-04-27","No","No","No","Internal"]
[null,null,null,null,11628,"57_30/4/2020 4:17:33 AM","2020-04-20","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","DG 1,2,& 3 -Lagging missing from FO filter","E/R - Aux. Engine","Eng. / Strg. Comp.","Behaviour Based,Equipment Related","10.27","Medium","","","Laggings were removed for cleaning. Same put back in place. ","2020-04-30","","Completed","2020-04-20","No","No","No","Internal"]
[null,null,null,null,11629,"57_30/4/2020 4:04:53 AM","2020-04-20","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Hydrophore pumps-suction /discharge gauges showing 4.5 bar. NRV for hyd tank not holding","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.1","Medium","","","NRV renewed. Now both pump discharge pressure reads zero while st/by","2020-05-20","","Completed","2020-04-30","No","No","No","Internal"]
[null,null,null,null,11630,"57_30/4/2020 4:36:47 AM","2020-04-20","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Spare ME piston- Open both clamps and inspect fretting at clamping area","E/R - Main Engine","Eng. / Strg. Comp.","Knowledge Based","10.1","Medium","","","Opened both clamps and inspected clamping area- found in good condition - No signs of fretting.","2020-05-20","","Completed","2020-04-23","No","No","No","Internal"]
[null,null,null,null,12122,"57_4/6/2020 04:02:23","2020-04-24","Defect","Ship Staff","Ship Staff Insp.","Fpk tk. gate v/v (450A) unable to be operated from main dk. (only manual op. for this v/v)","Hull & Tanks","Cargo / Ballast Systems","Equipment Related","8.11","Medium","","","On tank entry it was noted v/v stuck in position, v/v dismantled, found that gate flange was reversed (back to front) & open/shut hyd connections to hyd motor also reversed. v/v derusted, cleaned, painted & position of gate flange & hyd connections rectified. v/v now operating","2020-05-31","","Completed","2020-05-26","No","No","No","Internal"]
[null,null,null,null,12121,"57_2/6/2020 8:47:08 AM","2020-05-31","Defect","Ship Staff","Engineering Audit","ME Unit 2 liner and piston rings found scuffing heavily and worn out.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Unit 2 Cylinder lubrication increased. Pmax offset ME Unit 2 Piston and stuffing box renewed","2020-07-14","DSTA205039","Completed","2020-07-03","No","No","No","Internal","Spare liner will be supplied at Singapore on 2nd July."]
[null,null,null,null,12817,"57_24/6/2020 1:20:55 PM","2020-06-03","Defect","Ship Staff","Ship Staff Insp.","Jacket cooling water found leaking into fresh water generator evaporator","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.1","Medium","","","FWG isolated and evaporator pressure tested. Found one tube leaking- same plugged using brass plug. Pressure tested again and found satisfactory.","2020-07-05","NA","Completed","2020-06-04","No","No","No","Internal"]
[null,null,null,null,15934,"57_20/12/2020 11:23:46 AM","2020-07-30","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","CW pressure gauge defective","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Pressure gauge renewed.","2020-08-07","","Completed","2020-08-03","No","No","No","Internal"]
[null,null,null,null,15935,"57_20/12/2020 11:26:19 AM","2020-07-30","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Central cooling FW cooler no. # 1 & 2 foundation has salt deposit. Identify source & rectify","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","SW inlet Filter gaskets renewed and leak rectified.","2020-08-07","","Completed","2020-08-05","No","No","No","Internal"]
[null,null,null,null,15936,"57_20/12/2020 11:29:59 AM","2020-07-30","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Cooler no. 1 & 2 back flush sheet not updated for last back flush","Documentation","Cert. & Docu.","Human Error","10.1","Medium","","","Back flush date updated.","2020-08-07","","Completed","2020-07-31","No","No","No","Internal"]
[null,null,null,null,15937,"57_20/12/2020 11:32:41 AM","2020-07-30","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Motor shaft seal oil glass empty","Deck - Machinery","Eng. / Strg. Comp.","Equipment Related","6.13","Low","","","Oil topped up.","2020-08-07","","Completed","2020-08-01","No","No","No","Internal"]
[null,null,null,null,15938,"57_20/12/2020 11:34:46 AM","2020-07-30","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Oil traces near drain valve. Identify source & rectify","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Drain valve tightened and leak rectified.","2020-08-14","","Completed","2020-08-04","No","No","No","Internal"]
[null,null,null,null,15939,"57_20/12/2020 11:37:14 AM","2020-07-30","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","LO tank normal level to mark","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.1","Medium","","","LO tank normal level marked.","2020-07-31","","Completed","2020-07-31","No","No","No","Internal"]
[null,null,null,null,15940,"57_21/12/2020 11:10:00 AM","2020-07-30","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","COT 3P IG line blank plate not at stowage location","Deck - Pipe / Fittings","Cargo / Ballast Systems","Human Error","8.23","Medium","","","3P IG line blank plates secured back at stowage location","2020-08-07","","Completed","2020-07-31","No","No","No","Internal"]
[null,null,null,null,15941,"57_21/12/2020 11:15:57 AM","2020-07-30","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Compass deck-Spot rust spots on hinges, stanchions etc to derust & paint","Accommodation","General Appearance","Equipment Related","11.8","Low","","","Spot derusting and painting maintenance completed.","2020-08-30","","Completed","2020-08-06","No","No","No","Internal"]
[null,null,null,null,13849,"57_11/8/2020 10:02:00 AM","2020-08-04","Defect","Ship Staff","Ship Staff Insp.","DG #2 centrifuge filter base flange cracked","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Received new LO centrifugal filter fitted in place with small modification in pipe line connection. Now in operation and working satisfactory.","2021-03-31","","Completed","2021-02-18","No","No","No","Internal","Spare is ready at Singapore. Will be supplied during bunker call."]
[null,null,null,null,13851,"57_11/8/2020 10:08:23 AM","2020-08-04","Defect","Ship Staff","Ship Staff Insp.","PA system amplifer defective","Miscellaneous","Safety / LSA / FFA","Equipment Related","11.16","Low","","","Defective transistors in the amplifiers on both the systems renewed. Need to check system performance","2020-08-31","","Completed","2020-08-12","No","No","No","Internal"]
[null,null,null,null,13852,"57_19/8/2020 3:34:59 PM","2020-08-07","Defect","Ship Staff","Ship Staff Insp.","MF /HF Antenna was damaged during rough weather","Navigation - GMDSS & Communication","Communication","External Factors","","","","","Requisition DSTA205057 was supplied and defective MF/HF Antenna was renewed.","2020-08-15","DSTA205057","Completed","2020-08-13","No","No","No","Internal"]
[null,null,null,null,13853,"57_19/8/2020 3:41:46 PM","2020-08-07","Observation","Ship Staff","Ship Staff Insp.","Stbd Gangway :One shifting wire broken ,same to be renewed.","Miscellaneous","Safety / LSA / FFA","Equipment Related","5.47","Medium","","","Damaged shifting wire renewed with spare.","2020-08-15","NA","Completed","2020-08-10","No","No","No","Internal"]
[null,null,null,null,13855,"57_11/8/2020 10:10:31 AM","2020-08-08","Defect","Ship Staff","Ship Staff Insp.","Hotwell gauge glass leaking.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Gaugle glass renewed leak arrested.","2020-08-15","","Completed","2020-08-10","No","No","No","Internal"]
[null,null,null,null,13850,"57_19/8/2020 3:59:31 PM","2020-08-10","Observation","Ship Staff","Ship Staff Insp.","Gangway falls and shifting wires are in service since vessels delivery ( Installed On 27th April 2018), same to be renewed every 24M as per GSM SAFETY CIRCULAR/S-001-2019 - POINT NO 6","Miscellaneous","ISM Related","Equipment Related","5.47","Medium","","","Gangway Falls Renewed On 24th Oct 2020.","2020-12-31","DSTA-200175: Received ","Completed","2020-10-24","No","No","No","Internal"]
[null,null,null,null,13848,"57_19/8/2020 5:12:08 PM","2020-08-11","Observation","Ship Staff","Ship Staff Insp.","Echo Sounder Printer Thermal head is malfunctioning & requires replacement, as the data print is unreadabale.","Navigation - Echo Sounder / Speed Log","Navigation","Equipment Related","4.19","Low","","","Spares received and Echo Sounder Thermal Printer Head renewed.","2020-12-31","DSTA-205063-Received","Completed","2020-10-14","No","No","No","Internal"]
[null,null,null,null,14358,"57_14/9/2020 4:18:38 PM","2020-08-14","Observation","Ship Staff","Ship Staff Insp.","DG #1 and #3 T/C exh gas inlet temp gauge not working","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.33","High","","","DSTA200070 raised, cancelled from office. Requesition raised again DSTA210034, SPARES RECEIVED AT SINGAPORE, REPLACEMENT OF SENSOR IS GOING ON. COMPLETED.","2021-01-31","DSTA210034","Completed","2021-01-15","No","No","No","Internal","Will be supplied at Singapore during bunker call."]
[null,null,null,null,13854,"57_15/8/2020 2:06:29 PM","2020-08-15","Critical Equipment","Ship Staff","Ship Staff Insp.","Stbd lifeboat engine not starting","LSA / FFA","Safety / LSA / FFA","Equipment Related","10.6","Very High","","","Starting motor overhauled. engine tried out on both batteries, working satisfactory.","2020-08-15","","Completed","2020-08-15","No","No","No","Internal"]
[null,null,null,null,14363,"57_8/9/2020 6:38:38 AM","2020-08-20","Defect","Ship Staff","Ship Staff Insp.","DG #2 unit 1 fuel valve pocket sleeve o-ring damaged resulting in water leak","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Unit 1 fuel valve sleeve O-rings renewed with new spare","2020-08-31","","Completed","2020-08-22","No","No","No","Internal"]
[null,null,null,null,14357,"57_16/9/2020 11:43:27 PM","2020-08-23","Observation","Ship Staff","Ship Staff Insp.","Pilot ladder onboard  do not comply with GSM  Safety Flash 20120420","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.47","Medium","","","1 NEW PILOT LADDER SUPPIED -STBD SIDE PILOT LADDER RENEWED.","2021-02-28","DSTA210007","Completed","2021-01-20","No","No","No","Internal","Will be supplied at Singapore."]
[null,null,null,null,14364,"57_8/9/2020 6:43:20 AM","2020-08-24","Defect","Ship Staff","Ship Staff Insp.","# steam leaks in E/rm to be rectified","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Steam leaks rectified as the vessel was in port","2020-08-31","","Completed","2020-08-31","No","No","No","Internal"]
[null,null,null,null,14359,"57_16/9/2020 11:54:12 PM","2020-08-30","Critical Equipment,Observation","Ship Staff","Ship Staff Insp.","One tank overfill alarm light (Stbd side midhship / aft light) was not operational.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.14","Very High","","","Tank Overfill Alarm Light Renewed.","2020-12-31","DSTA200177:Requisition raised for spare horn and light.","Completed","2020-08-31","No","No","No","Internal"]
[null,null,null,null,14365,"57_8/9/2020 6:35:48 AM","2020-09-02","Defect","Ship Staff","Engineering Audit","ME Unit 7 FIVA accumulator found with 26 bars pressure","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Accumulator renewed with new spare","2020-09-05","","Completed","2020-09-03","No","No","No","Internal"]
[null,null,null,null,14360,"57_16/9/2020 11:47:46 PM","2020-09-09","Defect,Observation","Ship Staff","Ship Staff Insp.","The fabric material condition of the stretcher in Pumproom has deteriorated. Additionally, the straps were observed to be broken.","Miscellaneous","Safety / LSA / FFA","Equipment Related","5.2","Very High","","","New stretcher received and put  in service","2020-12-17","DSTA200182-Received","Completed","2020-10-14","No","No","No","Internal"]
[null,null,null,null,14361,"57_17/9/2020 12:00:49 AM","2020-09-10","Non Conformity,Observation","Ship Staff","Ship Staff Insp.","Working life vests not SOLAS Compliant.","LSA / FFA","Safety / LSA / FFA","Equipment Related,Knowledge Based","5.32","High","","","Requisition Received- New SOLAS Compliant Work Vest Used .","2020-12-10","DSTA-200178 -Received","Completed","2020-10-14","No","No","No","Internal"]
[null,null,null,null,14362,"57_17/9/2020 12:48:49 AM","2020-09-15","Defect,Observation","Ship Staff","Ship Staff Insp.","CCR remote ballast level readings are erratic , system requires to be rebooted occassionally .","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.18","High","","","one HPI-100 PCB renewed for bunker tanks, another PCB also renewed. Working satisfactory. Job order no: V-DSTA020978/21","2021-02-28","","Completed","2021-01-29","No","No","No","Internal","Spare will be supplied while passing Singapore around 25th Dec."]
[null,null,null,null,15295,"57_25/11/2020 5:12:34 PM","2020-09-17","Defect","Ship Staff","Ship Staff Insp.","Sea water leakage from main sea water pump #2","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Mechanical seal renewed. RO raised for spare seal.","2020-09-20","DSTA200204","Completed","2020-09-18","No","No","No","Internal"]
[null,null,null,null,15296,"57_25/11/2020 5:18:51 PM","2020-09-20","Critical Equipment","Ship Staff","Ship Staff Insp.","High expension foam system proportioner valve diaphgram damage","LSA / FFA","Safety / LSA / FFA","Industry Issue","","","","","Proportioner valve diaphgram renewed.","2020-09-30","","Completed","2020-09-23","No","No","No","Internal"]
[null,null,null,null,15297,"57_25/11/2020 5:22:22 PM","2020-09-22","Breakdown","Ship Staff","Ship Staff Insp.","ME unit no 2 exhaust valve not operating","E/R - Main Engine","Eng. / Strg. Comp.","Industry Issue","10.1","Medium","","","Unit no 2 exh valve,fiva valve,MPC,exhaust valve actuator, LO HP pipe renewed during trobleshooting. LO HP pipe found damaged.","2020-09-22","","Completed","2020-09-22","No","No","No","Internal"]
[null,null,null,null,15298,"57_25/11/2020 5:31:00 PM","2020-09-24","Defect","Ship Staff","Ship Staff Insp.","ME unit no & fuel oil leak off alarm getting activated","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.1","Medium","","","Distributer to fuel valve aft and middle pipe renewed. fwd pipe replaced with overhauled one. booster to distribution block pipe lapping carried out and leak rectified.","2020-09-25","","Completed","2020-09-24","No","No","No","Internal"]
[null,null,null,null,15299,"57_25/11/2020 5:33:52 PM","2020-10-04","Defect","Ship Staff","Ship Staff Insp.","ME unit no 3 FO HP pipe leaking from outer pipe (booster to distribution block)","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.1","Medium","","","Surface lapping carried out and pipe replaced with overhauled pipe.","2020-10-05","","Completed","2020-10-04","No","No","No","Internal"]
[null,null,null,null,15304,"57_25/11/2020 5:36:55 PM","2020-10-14","Defect","Ship Staff","Ship Staff Insp.","Main engine Aux Blower #2 was not operating due to main contactor holding coil failure.","E/R - Main Engine","Eng. / Strg. Comp.","Industry Issue","10.1","Medium","","","Main contactor renewed. Requesition raised for spare contactor.","2020-10-14","DSTA200213","Completed","2020-10-14","No","No","No","Internal"]
[null,null,null,null,15300,"57_25/11/2020 5:43:28 PM","2020-10-15","Defect","Ship Staff","Ship Staff Insp.","Various steam leaks- Above ico lube unit, Above ME SCR unit and 6K dump valve flanges","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Industry Issue","10.29","Medium","","","Gaskets renewed and leak rectified.","2020-10-20","","Completed","2020-10-16","No","No","No","Internal"]
[null,null,null,null,15301,"57_25/11/2020 5:46:53 PM","2020-10-19","Defect","Ship Staff","Ship Staff Insp.","Aft hydraulics LO leak from HP pipe flange inside steering gear room","Deck - Mooring Machinery","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","O ring renewed and leak rectified.","2020-10-20","","Completed","2020-10-20","No","No","No","Internal"]
[null,null,null,null,15302,"57_25/11/2020 8:59:42 PM","2020-10-26","Defect","Ship Staff","Ship Staff Insp.","Main engine unit no 6 FO HP pipe leak","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.19","Very High","","","FO pipe booster pump to distributor block removed. surface lapping carried out and leak rectified.","2020-10-27","","Completed","2020-10-26","No","No","No","Internal"]
[null,null,null,null,15303,"57_25/11/2020 9:08:05 PM","2020-10-27","Defect","Ship Staff","Ship Staff Insp.","Main engine unit #5 exhaust valve stroke was less compaired to other units","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.21","Medium","","","Exhaust valve spring air safety valve replaced with overhauled one.","2020-10-30","","Completed","2020-10-27","No","No","No","Internal"]
[null,null,null,null,15305,"57_25/11/2020 9:10:19 PM","2020-10-27","Defect","Ship Staff","Ship Staff Insp.","AE 3 fresh water attach pump seal leakage","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Seal renewed","2020-10-30","","Completed","2020-10-29","No","No","No","Internal"]
[null,null,null,null,15306,"57_25/11/2020 9:14:20 PM","2020-10-29","Defect","Ship Staff","Ship Staff Insp.","Valve remote control system hydraulic leak from valve control block flowmeter CL151","Deck - Machinery","Eng. / Strg. Comp.","Equipment Related","10.1","Medium","","","O ring renewed and leak rectified. Requestion raised for sapare o ring.","2020-11-02","DSTA200220","Completed","2020-10-31","No","No","No","Internal"]
[null,null,null,null,15289,"57_26/11/2020 7:03:32 PM","2020-11-13","Defect","Ship Staff","Ship Staff Insp.","Fwd Fire Wire Winch- Reduction Gear Defective","Deck - Mooring Machinery","Mooring","Equipment Related","","","","","Requisition DSTA200218 received at singapore on 14th Jan 2021.Reduction gear box overhauled and defective parts replaced. Fwd fire wire reel now in operatitional rediness.","2021-02-13","DSTA200218","Completed","2021-01-18","No","No","No","Internal","PO issued. Awaiting spare readiness."]
[null,null,null,null,15294,"57_26/11/2020 6:53:50 PM","2020-11-13","Defect","Ship Staff","Ship Staff Insp.","Pumproom & Engine room TRO- N (Neutralising agent tank) Level sensor defective.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","6.21","High","","","Both pump room and engine room level sensors replaced with spare new ones. Now both the level sensors are operational and showing the correct reading. Job order no: V-DSTA021223/21","2021-02-13","","Completed","2021-02-05","No","No","No","Internal","PO issued. Awaiting spare readiness."]
[null,null,null,null,15292,"57_26/11/2020 7:08:47 PM","2020-11-19","Defect","Ship Staff","Ship Staff Insp.","Mooring winch brake band regulating screws required to be freed up .","Deck - Mooring Machinery","Mooring","Equipment Related","","","",""," Mooring winch brake band regulating screws have been  lubricated and freed.","2021-02-19","","Completed","2020-11-29","No","No","No","Internal","Noted, update progress in weekly deck maintenance report."]
[null,null,null,null,15290,"57_26/11/2020 7:24:05 PM","2020-11-20","Observation","Ship Staff","Ship Staff Insp.","Two fire hoses observed to be leaking during pressure test.","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.35","Medium","","","Fire hose renewed.Defective fire hoses repaired and made good.","2021-02-20","","Completed","2021-11-22","No","No","No","Internal","Raise requisition after 31st Dec.  This can be closed, since it is not a defect. Spare rope tails will be supplied before expiry."]
[null,null,null,null,15291,"57_26/11/2020 7:13:54 PM","2020-11-20","Observation","Ship Staff","Ship Staff Insp.","Fixed Gas Detection System 30M Shore Service Not Carried Out.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","5.21","Medium","","","New RO DSTA210011 raised for 30M Shore Service of Fixed Gas Detection System  In Jan 2021. Planned to be conducted at vessels next call Singapore around 12th Jan 2021. SHORE TECHNICIAN ATTANDED VESSEL AT SINGAPORE ON 14TH JAN 2021 AND SHORE SERVICEING CARRIED OUT. ","2021-02-20","DSTA210011 & DSTA210012","Completed","2021-01-14","No","No","No","Internal","Awaiting quotation for sensor. For 30M service, raise requisition again after 31st Dec. Will arrange in Jan 2021, when vessel calls for bunkers."]
[null,null,null,null,15293,"57_26/11/2020 7:31:00 PM","2020-11-24","Observation","Ship Staff","Ship Staff Insp.","4S COT VAPOUR PRESSURE READING IN CCR IS ERRATIC.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.19","High","","","VAPOR PRESSURE SENSOR DISCONNECTED AND RESTARTED ,DEFECT OBSERVED TO BE RECTIFED.","2021-02-24","","Completed","2021-11-26","No","No","No","Internal","Raise requisition after 31st Dec."]
[null,null,null,null,15872,"57_2/12/2020 2:08:46 PM","2020-11-25","Defect","Ship Staff","Ship Staff Insp.","Fresh water genrator distillate pump leakage from seal","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Mechanical seal renewed and requesition raised for spare seal.","2020-11-27","DSTA200223","Completed","2020-11-26","No","No","No","Internal"]
[null,null,null,null,15867,"57_2/12/2020 2:19:50 PM","2020-11-26","Defect","Ship Staff","Ship Staff Insp.","Fresh water genrator ejector pump was not staring,found pump start delay time relay faulty","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.37","Medium","","","pump start delay time relay interchanged from winding heater delay time relay. requesition raised for relay to renew winding heater delay time relay. WORK COMPLETED, ON FWG EJECTOR PUMP AND IS WORKING SATISFACTORY, REQUISITION DSTA200223 PENDING, CLOSING DEFECT. ","2021-01-31","DSTA200223","Completed","2021-01-12","No","No","No","Internal"]
[null,null,null,null,15873,"57_14/12/2020 6:39:40 AM","2020-12-06","Defect","Ship Staff","Ship Staff Insp.","Stripping pump steam return line leakage near LO cooler and above soot tank.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.1","Medium","","","Both flanges gaskets renewed, leak rectified.","2020-12-10","","Completed","2020-12-07","No","No","No","Internal"]
[null,null,null,null,15868,"57_15/12/2020 8:55:32 AM","2020-12-08","Observation","Ship Staff","Ship Staff Insp.","Personal Multi gas detector MSA ALTAIR 4XR- Serial Number 06020321 is observed to be showing “Sensor Error” during its startup sequence .","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","5.23","Very High","","","Personal Multi gas detector MSA ALTAIR 4XR- Serial Number 06020321 has been replaced under IM&M Warrenty on 17th Dec 2020-Singapore Transit","2021-03-08","","Completed","2020-12-17","No","No","No","Internal","Spare supplied while passing Singapore. Close defect."]
[null,null,null,null,15869,"57_14/12/2020 22:45:31","2020-12-12","Defect","Ship Staff","Ship Staff Insp.","Fixed Gas Detection System GS5000: IG Blower area Oxygen sensor  is defective.Oxygen reading shows 25% Vol.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","5.21","Medium","","","Sensor interchanged with other area, found sensor defective.Requisition DSTA210006 raised in Jan 2021 for spare sensor. SPARES RECEIVED AT SINGAPORE, BUT BEFORE REPLACEMENT OF PARTS, VESSEL CHECKED SENSORS AGAIN AND NOW O2 READING IS SHOWING CORRECT.  RECEIVED SPARES KEPT FOR FUTURE USE, JOB COMPLETED","2021-03-12","DSTA210006","Completed","2021-01-15","No","No","No","Internal","Raise requisition ASAP to supply at Singapore bunker call."]
[null,null,null,null,15874,"57_14/12/2020 6:43:53 AM","2020-12-14","Defect","Ship Staff","Ship Staff Insp.","Sludge pump priming fresh water supply valve spindle sheared off.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Valve renewed.","2020-12-14","","Completed","2020-12-14","No","No","No","Internal"]
[null,null,null,null,15870,"57_14/12/2020 23:05:31","2020-12-15","Observation","Ship Staff","Ship Staff Insp.","IG line vent valve before deck seal observed to have a pneumatic leak.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.22","Very High","","","Pneumatic actuator overhauled and O Ring renewed, IG line vent valve pneumatic leak rectified.","2021-03-15","","Completed","2020-12-17","No","No","No","Internal","Raise this in email when you send UTI for calibration. Since this is not a defect,  not worth keeping in DDRL. Close this observation in DDRL."]
[null,null,null,null,15871,"57_15/12/2020 9:24:21 AM","2020-12-15","Defect","Ship Staff","Ship Staff Insp.","During inspection of ballast tank vent heads it was observed that the forepeak water ballast tank vent head, inner seal ring was found missing .The float is damaged and is misaligned.","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","Equipment Related","8.1","Very High","","","Requisition DSTA200196 received at Singapore on 14th Jan 21. Fpk WBT vent overhauled ,Float & seal ring renewed. Fpk vent in operational condition.","2021-03-15","DSTA200196","Completed","2021-01-22","No","No","No","Internal","Will be supplied at Singapore bunker call."]
[null,null,null,null,15942,"57_20/12/2020 11:49:57 AM","2020-12-18","Defect","Ship Staff","Ship Staff Insp.","ALL 3 COPT steam line supports found loose.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.1","Medium","","","Steam line supports alignened and tightened.","2020-12-20","","Completed","2020-12-19","No","No","No","Internal"]
[null,null,null,null,15933,"57_20/12/2020 12:05:34 PM","2020-12-20","Defect","Ship Staff","Ship Staff Insp.","Sea water seepage from LT cooler vent valve connection.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Vent valve connection renewed and leak rectified.","2020-12-31","","Completed","2020-12-28","No","No","No","Internal","Plan to rectify defect at Port stay in China."]
[null,null,null,null,16698,"57_5/1/2021 7:48:27 AM","2020-12-23","Defect","Ship Staff","Ship Staff Insp.","Aux Boiler No 1 water level gauge glass leakage","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.1","Medium","","","Gauge glass gaskets renewed and leak rectified.","2020-12-24","","Completed","2020-12-23","No","No","No","Internal"]
[null,null,null,null,16696,"57_5/1/2021 7:36:28 AM","2020-12-26","Defect","Ship Staff","Ship Staff Insp.","Low sea chest MGPS module TC2 defective","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.33","High","","","Module to renew. Requesition raised for spare, SPARES RECEIVED MGPS MODULE CARD REPLACED, DEFECT RECTIFIED, MGPS SYSTEM BACK TO NORMAL. ","2021-03-31","DSTA200251","Completed","2021-01-15","No","No","No","Internal","Will be supplied at Singapore on 13th Jan."]
[null,null,null,null,16697,"57_5/1/2021 7:40:53 AM","2020-12-28","Defect","Ship Staff","Ship Staff Insp.","PA System amplifier unit defective.","Elect. Mach. & Equip.","Communication","Equipment Related","10.33","High","","","Trobuleshooting in progress. SPARES RECEIVED AT SINGAPORE ON 14TH JAN 2021, VESSEL CHANGED ALL ELECTRICAL CARDS ON SYSTEM, PA SYSTEM BACK IN OPERATION, JOB COMPLED","2021-03-31","","Completed","2021-01-15","No","No","No","Internal","Locate equipment which is giving short circuit."]
[null,null,null,null,null,"57_13/1/2021 2:12:17 AM","2021-01-08","Breakdown","Ship Staff","Ship Staff Insp.","MCSW pump No 1 not operational due to falty VFD","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related",10.37,"Medium","Not Applicable","Not Applicable","VFD internal component got damaged. Requesition raised for same. DSTA210043, Need shore assitance for fault rectification, Need to land VFD at Singapore and receive it back after repairs. Management has decided to give new VFD, And for emerengy purposes one DOL is given at Singapore, DOL mounting stand  fabrication  is going on and job will get complete before month end. Once DOL in place we can close this job. DOL STARTER PANEL INSTALLED. PUMP TRIED OUT. ALL SATISFACTORY< PUMP NO-1 IS BACK IN USE.","2021-05-31","DSTA210043,","Completed","2021-04-29","No",null,null,"Internal"]
[null,null,null,null,17570,"57_13/1/2021 3:46:16 AM","2021-01-10","Defect","Ship Staff","Ship Staff Insp.","ME SCR blower sealing air line pressure regulator defective","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.1","Medium","","","Pressure regulator replaced with spare new one. Job order no: V-DSTA020948/21","2021-02-28","","Completed","2021-01-27","No","No","No","Internal"]
[null,null,null,null,null,"57_20/10/2019 4:54:32 PM","2021-01-12","Defect","Ship Staff","Ship Staff Insp.","BWTS unit, inside filter unit many cleaning nozzles found in siezed and worn out condition.","Deck - Machinery","Cargo / Ballast Systems","Equipment Related",6.21,"High","Not Applicable","Not Applicable","Spares received at Singapore on 5th march-2020, to be attended, vessel in progress of rectifing faults on No-2 Filter, Two new filters installed inside No-2 filter casing.VESSEL OPENED LOOP TWO FILTER AND CHANGED TWO FILTERS CARTRIDGE, ALL SEALING ARRANGEMENT FOR BACK FLUSH SYSTEM CHANGED , FILTER TRIED OUT ALL SATISFACTORY. VESSEL IS RAISING REQUISITION FOR SPARE NOZZLES AND SPARES FOR FILTERS","2021-05-31",null,"Completed","2021-04-25","No",null,null,"Internal"]
[null,null,null,null,16695,"57_5/1/2021 7:32:53 AM","2021-01-17","Defect","Ship Staff","Ship Staff Insp.","FWD ICCP not working","Hull & Tanks","Eng. / Strg. Comp.","Equipment Related","10.37","Medium","","","Job carried out by service engineer. faulty thyristor renewed. System is operational and back to normal. Job order no: V-DSTA022074/21","2021-03-31","","Completed","2021-03-25","No","No","No","Internal","Service engineer will be arranged at Singapore."]
[null,null,null,null,17884,"57_10/2/2021 4:08:13 PM","2021-02-05","Defect","Ship Staff","Ship Staff Insp.","Central FW cooler AFT #2 SW outlet pipe leakage at the instrument flange.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Removed the pipe and instrument flange. All the surfaces cleaned. New gasket joints put in place. The cooler pressure tested and observed no leakage from the flange. The flange observed to be erroded from inner side. Same cleaned and put back. RO raised for the same for future use. Job order : V-DSTA021222/21, Vessel received two flanges under requisition DSTA210045, And also vessel has rectified leak. Spare flanges will be use in future for same leak - At present we can decide job completed. ","2021-04-30","DSTA210045","Completed","2021-04-10","No","No","No","Internal","Spare already supplied to vessel on 1st April."]
[null,null,null,null,18103,"57_28/2/2021 12:31:05 PM","2021-02-26","Observation","Ship Staff","Ship Staff Insp.","HFO purifier supply pump #2 seal leakage to rectify and motor overhaul.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","The pump dismantled and inspected for any sign of seal damage, foundmechanical seal in damaged condition, same replaced with new one.\n\nThe pump bearing and rotors inspected, found in good condition.\n\nThe motor dismantled by ETO, both the bearings renewed. Stator and rotor observed to be in good condition.\n\nPump and motor boxed back with new coupling pad as it was not in place and found in broken small pieces. Job order no: V-DSTA021457/21\n\nNew teflon coupling pad made and fitted in place.\n\nThe pump tried out found working satisfactory. No abnormal noise, vibration and no seal leakage observed. Pump suction pr: 0.1 bar Discharge pr: 1.20 bar","2021-02-28","","Completed","2021-02-26","No","No","No","Internal"]
[null,null,null,null,18746,"57_14/4/2021 2:38:18 PM","2021-03-25","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Cooling fan for ER fan control panel not operational.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Cooling fan overhauled and now working satisfactory. ","2021-05-25","","Completed","2021-03-26","No","No","No","Internal"]
[null,null,null,null,18747,"57_14/4/2021 2:41:13 PM","2021-03-25","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Sewage treatment plant sludge recirculation not operational.","Documentation,E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Sewage treatment plant cleaned, Circulation pipe cleared, Operation checked all satisfactory","2021-04-05","","Completed","2021-04-01","No","No","No","Internal"]
[null,null,null,null,18748,"57_14/4/2021 2:43:29 PM","2021-03-25","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ER Bell book entries not complying with guidelines. Entries to be made as per guidelines given in the first page.","Documentation","Eng. / Strg. Comp.","Inappropriate Procedure","10.5","Low","","","All entries checked, and corrected, All engineers were shown what all entries are required and wording of entries explained","2021-04-05","","Completed","2021-04-01","No","No","No","Internal"]
[null,null,null,null,18476,"57_31/3/2021 2:36:10 PM","2021-03-30","Defect","Ship Staff","Ship Staff Insp.","Fresh Water generator salinometer defective, not showing any PPM reading.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.1","Medium","","","Vessel need to replace defective salinometer probe and meter to resolve fault. Vessel does not have spare salinometer on board requisition DSTA210081 raised for same. Vesel found one spare salinometer on board wich was replaced in place of defective salinometer. DSTA210081 has been approved by management will come on board in future. At present job completed. ","2021-06-30","DSTA210081","Completed","2021-04-09","No","No","No","Internal","One spare sensor was supplied to vessel in Jan 2020. Please check."]

{"sheet":"Calc","index":2,"n_rows":28,"n_cols":12,"rows_kept":28,"cut":false,"hidden":true,"merged":[]}
["Def_type","Def_cause","Equipments","VIQrefno","Observer_code"]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,"Dim itemSele As Long"]
[null,null,null,null,null,null,null,null,null,null,null,"   dim startRow as integer"]
[null,null,null,null,null,null,null,null,null,null,null,"   startRow=1"]
[null,null,null,null,null,null,null,null,null,null,null,"        For itemSele = 0 To ListBox1.ListCount - 1"]
[null,null,null,null,null,null,null,null,null,null,null,"        If ListBox1.Selected(itemSele) = True Then"]
[null,null,null,null,null,null,null,null,null,null,null,"        Worksheets(\"WorksheetName\").Range(\"A\" & startRow).Value = ListBox1.List(itemSele)"]
[null,null,null,null,null,null,null,null,null,null,null,"        startRow = startRow + 1"]
[null,null,null,null,null,null,null,null,null,null,null,"        End If"]
[null,null,null,null,null,null,null,null,null,null,null,"        Next"]
[null,null,null,null,null,null,null,null,null,null,null,"Dim LastRowA As String"]
[null,null,null,null,null,null,null,null,null,null,null,"        Dim itemSele As Long"]
[null,null,null,null,null,null,null,null,null,null,null,"       Dim startRow as integer"]
[null,null,null,null,null,null,null,null,null,null,null,"        LastRowA = ActiveSheet.Cells(Rows.count, \"A\").End(xlUp).row"]
[null,null,null,null,null,null,null,null,null,null,null,"        startQue = 0"]
[null,null,null,null,null,null,null,null,null,null,null,"        For itemSele = 0 To ListBox1.ListCount - 1"]
[null,null,null,null,null,null,null,null,null,null,null,"        For startRow = 1 To LastRowA"]
[null,null,null,null,null,null,null,null,null,null,null,"        If Worksheets(\"WorksheetName\").Range(\"A\" & startRow).Value = ListBox1.List(itemSele) Then"]
[null,null,null,null,null,null,null,null,null,null,null,"        ListBox1.Selected(itemSele) = True"]
[null,null,null,null,null,null,null,null,null,null,null,"        Exit For"]
[null,null,null,null,null,null,null,null,null,null,null,"        End If"]
[null,null,null,null,null,null,null,null,null,null,null,"        Next j"]
[null,null,null,null,null,null,null,null,null,null,null,"        Next"]
[null,null,null,null,null,null,null,null,null,null,null,"        End If"]

{"sheet":"Areaofobs","index":3,"n_rows":17,"n_cols":2,"rows_kept":17,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Cargo / Ballast Systems",11]
["Cert. & Docu.",2]
["Communication",6]
["Crew Management",3]
["Emgcy. Systems",13]
["Eng. / Strg. Comp.",14]
["General Appearance",15]
["Ice Opns.",17]
["ISM Related",7]
["ISPS Related",10]
["MARPOL Related",9]
["MLC Related",4]
["Mooring",12]
["Navigation",5]
["Safety / LSA / FFA",8]
["Structural Condn. / WT integrity ",16]

{"sheet":"Vessel_type","index":4,"n_rows":1,"n_cols":2,"rows_kept":1,"cut":false,"hidden":true,"merged":[]}
["Vessel_type","ID"]

{"sheet":"Deficiency_type","index":5,"n_rows":8,"n_cols":3,"rows_kept":8,"cut":false,"hidden":true,"merged":[]}
["TITLE","Type of deficiency_description","ID"]
["Breakdown",null,6]
["Critical Equipment",null,4]
["Defect",null,1]
["Guarantee Claim",null,8]
["Non Conformity",null,2]
["Observation",null,3]
["Other",null,7]

{"sheet":"VIQrefno","index":6,"n_rows":427,"n_cols":3,"rows_kept":427,"cut":false,"hidden":true,"merged":[]}
["VIQ_ref_no","Risk Value of observation","ID"]
["1.1","Low",8243]
["1.10","Low",8252]
["1.11","Low",8253]
["1.12","Low",8254]
["1.13","Low",8255]
["1.14","Low",8256]
["1.15","Low",8257]
["1.16","Low",8259]
["1.17","Low",8260]
["1.18","Low",8261]
["1.19","Low",8262]
["1.2","Low",8244]
["1.20","Low",8263]
["1.21","Low",8265]
["1.22","Low",8266]
["1.23","Low",8267]
["1.24","Low",8268]
["1.25","Low",8269]
["1.26","Low",8270]
["1.3","Low",8245]
["1.4","Low",8246]
["1.5","Low",8247]
["1.6","Low",8248]
["1.7","Low",8249]
["1.8","Low",8250]
["1.9","Low",8251]
["1.99","High",11258]
["10.1","Medium",8461]
["10.10","High",8470]
["10.11","Medium",8471]
["10.12","Very High",8472]
["10.13","Very High",8473]
["10.14","Medium",8474]
["10.15","Low",8475]
["10.16","Very High",8476]
["10.17","Very High",8477]
["10.18","High",8478]
["10.19","Very High",8479]
["10.2","Low",8462]
["10.20","High",8480]
["10.21","Medium",8481]
["10.22","Low",8482]
["10.23","Medium",8483]
["10.24","Low",8484]
["10.25","Very High",8485]
["10.26","High",8486]
["10.27","Medium",8487]
["10.28","Low",8488]
["10.29","Medium",8489]
["10.3","Medium",8463]
["10.30","High",8490]
["10.31","Very High",8491]
["10.32","Very High",8492]
["10.33","High",8493]
["10.34","High",8494]
["10.35","Very High",8495]
["10.36","Very High",8496]
["10.37","Medium",8497]
["10.38","Medium",8498]
["10.39","High",8499]
["10.4","High",8464]
["10.40","Medium",8500]
["10.41","Medium",8501]
["10.42","Medium",8502]
["10.43","Medium",8503]
["10.44","Medium",8504]
["10.45","Very High",8505]
["10.46","High",8506]
["10.47","Medium",8507]
["10.48","High",8508]
["10.49","Medium",8509]
["10.5","Low",8465]
["10.50","High",8510]
["10.51","Low",8511]
["10.52","Medium",8512]
["10.53","Medium",8513]
["10.54","High",8514]
["10.55","Low",8515]
["10.6","Very High",8466]
["10.7","Medium",8467]
["10.8","Medium",8468]
["10.9","Medium",8469]
["10.99","High",8516]
["11.1","High",8420]
["11.10","Medium",8429]
["11.11","Very High",8430]
["11.12","Low",8431]
["11.13","Low",8432]
["11.14","Medium",8433]
["11.15","Low",8434]
["11.16","Low",8435]
["11.17","Low",8436]
["11.2","Medium",8421]
["11.3","Medium",8422]
["11.4","Very High",8423]
["11.5","Medium",8424]
["11.6","Medium",8425]
["11.7","High",8426]
["11.8","Low",8427]
["11.9","Low",8428]
["11.99","High",8437]
["12.1","High",8438]
["12.10","High",8448]
["12.11","High",8449]
["12.12","High",8450]
["12.13","High",8451]
["12.14","High",8452]
["12.15","High",8453]
["12.16","High",8454]
["12.17","High",8455]
["12.18","High",8456]
["12.19","High",8457]
["12.2","High",8439]
["12.20","High",8458]
["12.21","High",8459]
["12.3","High",8441]
["12.4","High",8442]
["12.5","High",8443]
["12.6","High",8444]
["12.7","High",8445]
["12.8","High",8446]
["12.9","High",8447]
["12.99","High",8460]
["2.1","Very High",8296]
["2.1.9","Very High",11259]
["2.10","Medium",8304]
["2.11","Medium",8305]
["2.12","Low",8306]
["2.13","Low",8307]
["2.14","Low",8308]
["2.15","Low",8309]
["2.16","Medium",8310]
["2.2","Medium",8297]
["2.3","High",8295]
["2.4","Medium",8298]
["2.5","Medium",8299]
["2.6","Low",8300]
["2.7","High",8301]
["2.8","High",8302]
["2.9","Medium",8303]
["2.99","High",8311]
["3.1","High",8312]
["3.2","Very High",8313]
["3.3","High",8314]
["3.4","Low",8294]
["3.5","Medium",8315]
["3.6","High",8316]
["3.7","Very High",8317]
["3.8","Very High",8318]
["3.99","High",8319]
["4.1","High",8320]
["4.10","High",8329]
["4.11","Medium",8330]
["4.12","Very High",8331]
["4.13","Very High",8332]
["4.14","Very High",8333]
["4.15","Very High",8334]
["4.16","Very High",8335]
["4.17","Very High",8336]
["4.18","Very High",8337]
["4.19","Low",8338]
["4.2","Medium",8321]
["4.20","Very High",8339]
["4.21","High",8340]
["4.22","Low",8341]
["4.23","High",8342]
["4.24","High",8343]
["4.25","Low",8344]
["4.26","Low",8345]
["4.27","High",8346]
["4.3","Medium",8322]
["4.4","High",8323]
["4.5","Very High",8324]
["4.6","Medium",8325]
["4.7","High",8326]
["4.8","Medium",8327]
["4.9","Medium",8328]
["4.99","High",8347]
["5.1","Very High",8517]
["5.10","High",8526]
["5.11","Low",8527]
["5.12","Medium",8528]
["5.13","High",8529]
["5.14","Very High",8530]
["5.15","Medium",8531]
["5.16","Very High",8532]
["5.17","Very High",8533]
["5.18","High",8534]
["5.19","Medium",8535]
["5.2","Very High",8518]
["5.20","Medium",8536]
["5.21","Medium",8537]
["5.22","High",8539]
["5.23","Very High",8540]
["5.24","Very High",8541]
["5.25","Medium",8542]
["5.26","Medium",8543]
["5.27","Medium",8544]
["5.28","Very High",8545]
["5.29","High",8546]
["5.3","Low",8519]
["5.30","High",8547]
["5.31","High",8548]
["5.32","High",8549]
["5.33","High",8550]
["5.34","Low",8551]
["5.35","Medium",8552]
["5.36","Low",8553]
["5.37","Low",8554]
["5.38","High",8555]
["5.39","Very High",8556]
["5.4","High",8520]
["5.40","Very High",8557]
["5.41","Very High",8558]
["5.42","Medium",8559]
["5.43","High",8560]
["5.44","High",8561]
["5.45","Medium",8564]
["5.46","Medium",8565]
["5.47","Medium",8566]
["5.48","Medium",8567]
["5.5","Low",8521]
["5.6","Low",8522]
["5.7","Medium",8523]
["5.8","Medium",8524]
["5.9","Very High",8525]
["5.99","High",8568]
["6.1","Medium",8348]
["6.10","Low",8357]
["6.11","High",8358]
["6.12","Medium",8359]
["6.13","Low",8360]
["6.14","High",8361]
["6.15","High",8362]
["6.16","Very High",8363]
["6.17","Very High",8364]
["6.18","Medium",8365]
["6.19","Low",8366]
["6.2","High",8349]
["6.20","Medium",8367]
["6.21","High",8368]
["6.22","Medium",8369]
["6.3","Low",8350]
["6.4","High",8351]
["6.5","Medium",8352]
["6.6","Medium",8353]
["6.7","High",8354]
["6.8","High",8355]
["6.9","Low",8356]
["6.99","High",8370]
["7.1","High",8371]
["7.10","High",8380]
["7.11","High",8381]
["7.12","High",8382]
["7.13","Medium",8383]
["7.14","Medium",8384]
["7.15","High",8385]
["7.16","High",8386]
["7.17","High",8387]
["7.2","High",8372]
["7.3","Low",8373]
["7.4","Low",8374]
["7.5","Low",8375]
["7.6","Medium",8376]
["7.7","Low",8377]
["7.8","High",8378]
["7.9","High",8379]
["7.99","High",8388]
["8.1","Very High",8569]
["8.10","Very High",8578]
["8.100","Low",11227]
["8.101","Medium",11228]
["8.102","Low",11229]
["8.103","Low",11230]
["8.104","Low",11231]
["8.105","Medium",11232]
["8.106","Medium",11233]
["8.107","Low",11234]
["8.108","High",11235]
["8.109","Very High",11236]
["8.11","Medium",8579]
["8.110","High",11237]
["8.111","Medium",11238]
["8.112","High",11239]
["8.113","Medium",11240]
["8.114","Low",11241]
["8.115","High",11242]
["8.116","Medium",11243]
["8.117","Medium",11244]
["8.118","Medium",11245]
["8.119","High",11246]
["8.12","Medium",8580]
["8.120","High",11247]
["8.121","Medium",11248]
["8.122","High",11249]
["8.123","High",11250]
["8.124","Low",11251]
["8.125","High",11252]
["8.126","Medium",11253]
["8.127","Medium",11254]
["8.13","Medium",8581]
["8.14","Very High",8582]
["8.15","High",8583]
["8.16","Very High",8584]
["8.17","Low",8585]
["8.18","High",8586]
["8.19","High",8587]
["8.199","High",11255]
["8.2","Medium",8570]
["8.20","Medium",8588]
["8.21","High",8589]
["8.22","Very High",8590]
["8.23","Medium",8591]
["8.24","Medium",8592]
["8.25","Very High",8593]
["8.26","High",8594]
["8.27","Medium",8595]
["8.28","Medium",8596]
["8.29","High",8598]
["8.3","Very High",8571]
["8.30","High",8599]
["8.31","High",8600]
["8.32","Low",8601]
["8.33","Medium",8602]
["8.34","High",8603]
["8.35","Medium",8604]
["8.36","Medium",8605]
["8.37","High",8607]
["8.38","Medium",8608]
["8.39","Medium",8609]
["8.4","Medium",8572]
["8.40","High",8610]
["8.41","Medium",8611]
["8.42","Medium",8612]
["8.43","Very High",8613]
["8.44","High",8615]
["8.45","High",8616]
["8.46","Very High",8617]
["8.47","Very High",8618]
["8.48","Medium",8619]
["8.49","High",8620]
["8.5","Very High",8573]
["8.50","Medium",8621]
["8.51","Low",8622]
["8.52","Low",8623]
["8.53","Low",8624]
["8.54","High",8625]
["8.55","Low",11182]
["8.56","Medium",11183]
["8.57","Medium",11184]
["8.58","High",11185]
["8.59","High",11186]
["8.6","Medium",8574]
["8.60","High",11187]
["8.61","Medium",11188]
["8.62","Very High",11189]
["8.63","High",11190]
["8.64","Medium",11191]
["8.65","Low",11192]
["8.66","High",11193]
["8.67","High",11194]
["8.68","High",11195]
["8.69","Medium",11196]
["8.7","High",8575]
["8.70","Medium",11197]
["8.71","Very High",11198]
["8.72","Medium",11199]
["8.73","Medium",11200]
["8.74","High",11201]
["8.75","Medium",11202]
["8.76","Medium",11203]
["8.77","Medium",11204]
["8.78","Medium",11205]
["8.79","Medium",11206]
["8.8","Medium",8576]
["8.80","Medium",11207]
["8.81","Low",11208]
["8.82","Medium",11209]
["8.83","Low",11210]
["8.84","Low",11211]
["8.85","Medium",11212]
["8.86","Medium",11213]
["8.87","Medium",11214]
["8.88","Low",11215]
["8.89","High",11216]
["8.9","High",8577]
["8.90","High",11217]
["8.91","High",11218]
["8.92","Medium",11219]
["8.93","Low",11220]
["8.94","Low",11221]
["8.95","Medium",11222]
["8.96","Medium",11223]
["8.97","Low",11224]
["8.98","High",11225]
["8.99","Medium",11226]
["9.1","Low",8390]
["9.10","Medium",8399]
["9.11","Medium",8400]
["9.12","Medium",8401]
["9.13","Low",8402]
["9.14","Medium",8403]
["9.15","Medium",8404]
["9.16","High",8405]
["9.17","High",8406]
["9.18","Low",8407]
["9.19","Low",8408]
["9.2","Very High",8391]
["9.20","Medium",8409]
["9.21","Medium",8410]
["9.22","Low",8411]
["9.23","Low",8412]
["9.24","Medium",8413]
["9.25","Low",8414]
["9.26","Low",8415]
["9.27","Low",8416]
["9.28","Medium",8417]
["9.29","Low",8418]
["9.3","Very High",8392]
["9.4","High",8393]
["9.5","High",8394]
["9.6","Low",8395]
["9.7","Medium",8396]
["9.8","Medium",8397]
["9.9","Medium",8398]
["9.99","High",8419]

{"sheet":"Equipment_list","index":7,"n_rows":28,"n_cols":3,"rows_kept":28,"cut":false,"hidden":true,"merged":[]}
["TITLE","Equipment_list_description","ID"]
["Accommodation",null,12]
["Cargo Mach.",null,13]
["Critical Equip.",null,16]
["Deck - Machinery",null,18]
["Deck - Mooring Machinery",null,15]
["Deck - Pipe / Fittings",null,20]
["Documentation",null,21]
["E/R - Air Comp.",null,8]
["E/R - Aux. Engine",null,4]
["E/R - Aux. Mach.",null,7]
["E/R - Boiler",null,5]
["E/R - Main Engine",null,3]
["E/R - Pipes/ valves & fittings",null,9]
["E/R - Pumps",null,32]
["E/R - Purifier",null,6]
["Elect. Mach. & Equip.",null,10]
["Hull & Tanks",null,19]
["Inert Gas",null,14]
["LSA / FFA",null,17]
["Miscellaneous",null,22]
["Navigation - DGPS / EPFS / AIS",null,28]
["Navigation - ECDIS",null,25]
["Navigation - Echo Sounder / Speed Log",null,26]
["Navigation - GMDSS & Communication",null,23]
["Navigation - Others",null,11]
["Navigation - RADAR",null,24]
["Navigation - VDR / BNWAS",null,30]

{"sheet":"PSC_MOU","index":8,"n_rows":11,"n_cols":3,"rows_kept":11,"cut":false,"hidden":true,"merged":[]}
["TITLE","PSC_MOU_description","ID"]
["Asia and the Pacific",null,2]
["Caribbean",null,4]
["Europe and the North Atlantic",null,1]
["Latin America",null,3]
["The Black Sea region",null,6]
["The Indian Ocean",null,8]
["The Mediterranean",null,7]
["The Riyadh MoU",null,9]
["USCG",null,10]
["West and Central Africa",null,5]

{"sheet":"Inspection_type","index":9,"n_rows":13,"n_cols":2,"rows_kept":13,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Bunkering Audit",14]
["Cargo Audit",17]
["Engineering Audit",16]
["ISM Audit",2]
["ISPS Audit",3]
["IT Audit",10]
["MLC Audit",1]
["Mooring Audit",9]
["Nav Audit / Verification",8]
["Onboard Training",18]
["Ship Staff Insp.",15]
["Suptd. Insp.",13]

{"sheet":"Deficiency_Cause","index":10,"n_rows":8,"n_cols":3,"rows_kept":8,"cut":false,"hidden":true,"merged":[]}
["TITLE","Deficiency_Cause_description","ID"]
["Behaviour Based",null,1]
["Equipment Related",null,4]
["External Factors",null,5]
["Human Error",null,7]
["Inappropriate Procedure",null,8]
["Industry Issue",null,6]
["Knowledge Based",null,3]

{"sheet":"Observer_code","index":11,"n_rows":3,"n_cols":3,"rows_kept":3,"cut":false,"hidden":true,"merged":[]}
["TITLE","Observer_code_description","ID"]
["Owner / Marine / Tech. Suptd.",null,3]
["Ship Staff",null,2]

{"sheet":"Status_code","index":12,"n_rows":6,"n_cols":3,"rows_kept":6,"cut":false,"hidden":true,"merged":[]}
["TITLE","Status_code_description","ID"]
["Completed",null,6]
["Deferred to D D",null,5]
["In progress",null,3]
["Not Started",null,2]
["Waiting spare",null,4]

{"sheet":"PSC_ref_no","index":13,"n_rows":19,"n_cols":2,"rows_kept":19,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Alarms",9]
["Cargo operations including equipment",7]
["Certificates & Documentation",2]
["Dangerous Goods",13]
["Emergency Systems",5]
["Fire safety",8]
["ISM",16]
["ISPS",17]
["Life saving appliances",12]
["MLC, 2006",18]
["Other",19]
["Pollution Prevention",15]
["Propulsion and auxiliary machinery",14]
["Radio communication",6]
["Safety of Navigation",11]
["Structural condition",3]
["Water/Weathertight condition",4]
["Working and Living Conditions",10]

{"sheet":"Risk_value_of_obs","index":14,"n_rows":1,"n_cols":2,"rows_kept":1,"cut":false,"hidden":true,"merged":[]}
["Risk Value of observation","ID"]

{"sheet":"Year","index":15,"n_rows":18,"n_cols":1,"rows_kept":18,"cut":false,"hidden":true,"merged":[]}
["Year"]
[2014]
[2015]
[2016]
[2017]
[2018]
[2019]
[2020]
[2021]
[2022]
[2023]
[2024]
[2025]
[2026]
[2027]
[2028]
[2029]
[2030]

{"sheet":"Month","index":16,"n_rows":13,"n_cols":1,"rows_kept":13,"cut":false,"hidden":true,"merged":[]}
["Month"]
["Jan"]
["Feb"]
["Mar"]
["Apr"]
["May"]
["Jun"]
["Jul"]
["Aug"]
["Sep"]
["Oct"]
["Nov"]
["Dec"]

{"sheet":"Date_","index":17,"n_rows":32,"n_cols":1,"rows_kept":32,"cut":false,"hidden":true,"merged":[]}
["Date"]
["01"]
["02"]
["03"]
["04"]
["05"]
["06"]
["07"]
["08"]
["09"]
[10]
[11]
[12]
[13]
[14]
[15]
[16]
[17]
[18]
[19]
[20]
[21]
[22]
[23]
[24]
[25]
[26]
[27]
[28]
[29]
[30]
[31]

{"sheet":"Sheet1","index":18,"n_rows":24,"n_cols":6,"rows_kept":24,"cut":false,"hidden":true,"merged":[]}
[]
[null,"ID","E",null,"Date Recorded",1]
[null,"UNIQUE ID","F",null,"Type of Deficiency",2]
[1,"Date Recorded","G",null,"Observer code",3]
["ignore","Vessel Type","H",null,"Type of Inspection",4]
[null,"Internal / External","I",null,"Description of Deficiency",5]
[null,"Drydock","J",null,"Equipment Categories",6]
[null,"Information Sharing","K",null,"Area of Observation",7]
[null,"Critical_item","L",null,"Deficiency Cause",8]
[null,"Deficiency Type","M",null,"VIQ Ref Number",9]
[null,"Deficiency Cause","N",null,"Risk Value of Obs",10]
[null,"Inspection Type","O",null,"PSC Ref Number",11]
[null,"Equipments","P",null,"PSC MOU ID",12]
[null,"VIQ Reference Number","Q",null,"Action Taken or Required",13]
[null,"Risk Value of the observation","R",null,"Target Date",14]
[null,"PSC Reference Number","S",null,"PO Ref No.",15]
[null,"PSC MOU","T",null,"Status Code",16]
[null,"Observer Code","U",null,"Date Completed",17]
[null,"Target Date","V",null,"Drydock",18]
[null,"Status Code","W",null,"Info Sharing",19]
[null,"Description of Deficiency","X",null,"Critical Item Flag",20]
[null,"Action taken / required","Y",null,"Audit Type",21]
[null,"PO ref no","Z"]
[null,"Date completed","AA"]

{"sheet":"Ship_information","index":19,"n_rows":2,"n_cols":3,"rows_kept":2,"cut":false,"hidden":true,"merged":[]}
["Ship_ID","Ship_Name","FILE_NAME"]
["57","DHT STALLION (26-04-2021)","57_1619428518417.xlsm"]

{"sheet":"External_Deficiency_type","index":20,"n_rows":5,"n_cols":3,"rows_kept":5,"cut":false,"hidden":true,"merged":[]}
["TITLE","Type of deficiency_description","ID"]
["Condn of Class / Memo",null,5]
["Defect",null,1]
["Non Conformity",null,2]
["Observation",null,3]

{"sheet":"External_Inspection_type","index":21,"n_rows":11,"n_cols":2,"rows_kept":11,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Cargo Audit",17]
["Flag State Insp.",5]
["ISM Audit",2]
["ISPS Audit",3]
["MLC Audit",1]
["Nav Audit / Verification",8]
["OM Insp. (Eg. SIRE / CDI etc.)",6]
["Others (Eg. Insurance etc.)",12]
["PSC Inspection",4]
["Terminal Insp.",11]

{"sheet":"External_Observer_code","index":22,"n_rows":7,"n_cols":3,"rows_kept":7,"cut":false,"hidden":true,"merged":[]}
["TITLE","Observer_code_description","ID"]
["Class Surveyor",null,4]
["FSC Inspector",null,5]
["Others (Eg. Insurance etc.)",null,9]
["PSC Insp.",null,6]
["SIRE / CDI Insp.",null,8]
["Terminal Insp.",null,7]

{"sheet":"Sheet Version","index":23,"n_rows":2,"n_cols":2,"rows_kept":2,"cut":false,"hidden":true,"merged":[]}
["Version","Title"]
["2.0","Version 2.0"]