{"text_format":"1","workbook":"xlsx","n_sheets":24,"sheets":["Mainsheet","Completed","Calc","Areaofobs","Vessel_type","Deficiency_type","VIQrefno","Equipment_list","PSC_MOU","Inspection_type","Deficiency_Cause","Observer_code","Status_code","PSC_ref_no","Risk_value_of_obs","Year","Month","Date_","Sheet1","Ship_information","External_Deficiency_type","External_Inspection_type","External_Observer_code","Sheet Version"],"not_rendered":{"charts":0,"images":5,"macros":1,"external_links":0,"defined_names":12,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Mainsheet","index":0,"n_rows":32,"n_cols":28,"rows_kept":32,"cut":false,"hidden":false,"merged":[[10,8,10,9],[10,12,10,13],[12,6,12,27],[8,6,8,27]]}
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,"Defect - Damage Monitoring Sheet"]
[]
[null,null,null,null,null,null,null,"Date of Report","29-May-2021",null,null,"Ship Name","RESPECT (29-04-2021)"]
[]
[null,null,null,null,null,null,"VERSION : 2.0"]
[]
[]
[]
[null,null,null,null,"ID","UNIQUE ID","Date Recorded","Type of Deficiency","Observer code","Type of Inspection","Description of Deficiency","Equipment Categories","Area of Observation","Deficiency Cause","VIQ Ref Number","Risk Value of Obs","PSC Ref Number","PSC MOU ID","Action Taken or Required","Target Date","PO Ref No.","Status Code","Date Completed","Drydock","Info Sharing","Critical Item","Audit Type","Superintendent Remarks"]
[null,null,null,null,18859,"49_28/4/2021 11:14:35 AM","2021-04-17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Pump room blower casing to be wire brushed and painted","Deck - Machinery","General Appearance","Equipment Related","11.3","Medium","","","Pump room blower casing to be derusted/painted","2021-06-16","","Not Started",null,"No","No","No","Internal"]
[null,null,null,null,18860,"49_28/4/2021 11:16:48 AM","2021-04-17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Monkey Island mast foundation plates of the various lights to be repaired. ","Navigation - Others","Navigation","Equipment Related","4.8","Medium","","","Derusting and renewal of wasted foundation plates","2021-05-16","","Not Started",null,"No","No","No","Internal"]
[null,null,null,null,18863,"49_28/4/2021 11:37:26 AM","2021-04-17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","New flush systems procured during the docking to be installed in the cabins where these are defective","Accommodation","MLC Related","Equipment Related","11.13","Low","","","New flush systems procured in DD. New system to be installed in cabins","2021-06-16","","In progress",null,"No","No","No","Internal"]
[null,null,null,null,18865,"49_28/4/2021 11:44:35 AM","2021-04-17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","All spare parts to be squared up and inventories updated","Miscellaneous","General Appearance","Behaviour Based","11.12","Low","","","All stores to be squared up and inventory to be updated.","2021-07-16","","In progress",null,"No","No","No","Internal"]
[null,null,null,null,18870,"49_28/4/2021 2:50:09 PM","2021-04-17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","FWG ejector pump pipeline to be modified to install the filters.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Ejector pump no 2 has been installed with filter. Pump working in satisfactory condition. No 1 pump filter installation inprogress ","2021-06-17",null,"In progress",null,"No","No","No","Internal"]
[null,null,null,null,18871,"49_28/4/2021 2:52:37 PM","2021-04-17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Steam traps in engine room found leaking. All steam traps to be overhauled. ","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","steam traps to overhaul","2021-07-17","","In progress",null,"No","No","No","Internal"]
[null,null,null,null,18873,"49_28/4/2021 3:02:21 PM","2021-04-17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Engine room vent fan rooms to be cleaned and painted. ","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","area to clean and paint","2021-07-17","","In progress",null,"No","No","No","Internal"]
[null,null,null,null,18875,"49_28/4/2021 3:19:15 PM","2021-04-17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Some LED lights were found installed without the modifications advised as per safety circular 108. All these fittings to be modified in line with the circular (chocks and capacitors to be removed). ","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related",10.37,"Medium","Not Applicable","Not Applicable","modification to continue","2021-07-17","RESP210160","In progress",null,"No","No","No","Internal"]
[null,null,null,null,18880,"49_28/4/2021 3:15:36 PM","2021-04-17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","There are many motors pending for overhaul. These are to be overhauled on a priority basis.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.37","Medium","","","motors to overhaul","2021-07-17","","In progress",null,"No","No","No","Internal"]
[null,null,null,null,null,"49_06/06/2021 8:50:54 PM","2021-05-10","Observation","Ship Staff","Ship Staff Insp.","COT 5C fwd cow machine leak to be arrested","Cargo Mach.","Cargo / Ballast Systems","Equipment Related",8.34,"High","Not Applicable","Not Applicable","COW machine to be opened up and overhauled. Damaged parts to be replaced with new spares on board. If spare parts not available then RO to raised for necessary spare parts.","2021-07-10",null,"Not Started",null,"No",null,null,"Internal"]
[null,null,null,null,null,"49_06/06/2021 3:19:54 PM","2021-05-12","Defect","Ship Staff","Ship Staff Insp.","MGPS system line flow meter found defective","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","flow meter removed and dismantled, found beyond repair, Reqn RESP210169 raised for new flowmeter","2021-09-01","RESP210169","Waiting spare",null,"No",null,null,"Internal"]
[null,null,null,null,null,"49_06/06/2021 9:01:39 PM","2021-05-13","Observation","Ship Staff","Ship Staff Insp.","Leaks from foam monitor to be rectified, adjacent to Stbd life boat at break of accommodation","LSA / FFA","Safety / LSA / FFA","Equipment Related",5.35,"Medium","Not Applicable","Not Applicable","Foam monitor to be opened up and O-rings to be replaced. Monitor to be tested for operation and leaks after overhauling.","2021-07-13",null,"In progress",null,"No",null,null,"Internal"]
[null,null,null,null,null,"49_06/06/2021 3:27:07 PM","2021-05-15","Defect","Ship Staff","Ship Staff Insp.","Stern tube system pump not in auto stby mode ","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","troubelshooting carried out, found flowswitch not working. Flow switch dismantled, found spring damage. RESP2101175 raised for new spare ","2021-09-01","RESP210175","Waiting spare",null,"No",null,null,"Internal"]
[null,null,null,null,null,"49_06/06/2021 3:32:56 PM","2021-05-18","Defect","Ship Staff","Ship Staff Insp.","Main Engine alpha lub pump unit tank heater non working","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","heater checked, found low insulation RESP210176 raised for new heater","2021-08-01","RESP210176","Waiting spare",null,"No",null,null,"Internal"]
[null,null,null,null,null,"49_06/06/2021 4:54:06 PM","2021-05-30","Critical Equipment","Ship Staff","Ship Staff Insp.","Air horn CO2 system -E/R Bottom platform stbd side found partly damage","LSA / FFA","Eng. / Strg. Comp.","Equipment Related",null,null,"Not Applicable","Not Applicable","RESP210184 raised for new spare horn","2021-08-01","RESP210184","Waiting spare",null,"No",null,null,"Internal"]

{"sheet":"Completed","index":1,"n_rows":427,"n_cols":28,"rows_kept":427,"cut":false,"hidden":false,"merged":[[10,8,10,9],[10,12,10,13],[12,6,12,27],[8,6,8,27]]}
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,"Defect - Damage Monitoring Sheet"]
[]
[null,null,null,null,null,null,null,"Date of Report","29-May-2021",null,null,"Ship Name","RESPECT (29-04-2021)"]
[]
[null,null,null,null,null,null,"VERSION : 2.0"]
[]
[]
[]
[null,null,null,null,"ID","UNIQUE ID","Date Recorded","Type of Deficiency","Observer code","Type of Inspection","Description of Deficiency","Equipment Categories","Area of Observation","Deficiency Cause","VIQ Ref Number","Risk Value of Obs","PSC Ref Number","PSC MOU ID","Action Taken or Required","Target Date","PO Ref No.","Status Code","Date Completed","Drydock","Info Sharing","Critical Item","Audit Type","Superintendent Remarks"]
[null,null,null,null,4988,"49_25/10/2019 3:33:50 AM","2018-08-09","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Heavy rust on main and return Hydraulic main line.","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.4","Very High","","","All mooring winches branch lines hydo blasted and leaking ones repaired.Pending is the main hydraulic line from fwd to aft.Planned to start the job after departure Long Beach.","2019-01-31","","Completed","2019-03-01","No","No","No","Internal"]
[null,null,null,null,5044,"49_26/10/2019 6:00:42 AM","2018-08-09","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Toilet flush lever damaged in 4th engineer and master's cabin.","Accommodation","MLC Related","Equipment Related","11.13","Low","","","Toilet flush lever renewed in 4th engineer and maste's cabin.","2018-11-08","","Completed","2019-05-20","No","No","No","Internal"]
[null,null,null,null,4966,"49_25/10/2019 2:01:42 AM","2018-09-12","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Deck maintenance from Light post stbd fwd to MW2 to be derusted and painted,30% completed from last inspection.","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.4","Very High","","","Deck maintenance from Light post stbd fwd to MW2 to be derusted and full coat painted.","2019-01-31","","Completed","2019-01-28","No","No","No","Internal"]
[null,null,null,null,4982,"49_25/10/2019 3:05:33 AM","2018-09-12","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ER exhaust pipeline for Boiler and EGB and the insulation behind to be cleaned","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.12","Very High","","","Pipelines and ductings cleaned and laggings renewed as necessary","2018-10-12","","Completed","2019-02-22","No","No","No","Internal"]
[null,null,null,null,4986,"49_25/10/2019 3:25:09 AM","2018-09-12","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","COW machines on deck and the isolation valve for the tanks 2,3,4,5, to be de rusted and painted.","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.4","Very High","","","De- rusting near COW branch lines for 1,,2,3,4 across completed,rest in progress.","2019-02-28","","Completed","2019-02-27","No","No","No","Internal"]
[null,null,null,null,4987,"49_25/10/2019 3:28:59 AM","2018-09-12","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Cow branch pipelines to be deruted and painted.","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.4","Very High","","","De-rusting near 1P,1S,2P,3P & 3S COT in progress","2019-01-31","","Completed","2019-02-27","No","No","No","Internal"]
[null,null,null,null,4989,"49_25/10/2019 3:39:01 AM","2018-09-12","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Hydraulic valves for thr pump room,828 found small LO leakage from Actuators.To confirm the seal kit and attened.","Cargo Mach.","Emgcy. Systems","Equipment Related","8.44","High","","","Currently there is no leakage, valve operated and verified.","2019-03-31","","Completed","2019-03-11","No","No","No","Internal"]
[null,null,null,null,4996,"49_25/10/2019 6:35:48 AM","2018-09-12","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","CO2 mushroom exhaust fan to be opened up and valve lied to be derusted and painted.  ","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.4","Very High","","","De- rusted and painted.","2019-02-28","","Completed","2019-03-17","No","No","No","Internal"]
[null,null,null,null,5001,"49_25/10/2019 6:52:29 AM","2018-09-12","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Ballast tank Vent head maintenance for the spare Vent head kept on poop side of the deck to be carried out.Good condition vent head to be kept as spare and protected.","Miscellaneous","General Appearance","Inappropriate Procedure","11.4","Very High","","","All the vents kept on poop deck are heavily rusted.They are beyonds repairs as the de- rusting will increase the opening.","2019-01-31","","Completed","2019-03-31","No","No","No","Internal"]
[null,null,null,null,5006,"49_25/10/2019 7:17:34 AM","2018-09-12","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Stern View paint for the ship name and IMO No. to be painted.","Hull & Tanks","General Appearance","External Factors","11.4","Very High","","","vessel expecting name change therefore the job will be carried out after the change of name.","2019-01-31","","Completed","2019-04-01","No","No","No","Internal"]
[null,null,null,null,5047,"49_26/10/2019 6:24:10 AM","2018-09-12","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","No.2 & 3 COP pneumatic discharged valve not functional remotely need to attend in emergency.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.44","High","","","Opened and inspected. Repaired carried out, Operational.","2018-10-12","NERI180282","Completed","2019-05-18","No","No","No","Internal"]
[null,null,null,null,5063,"49_26/10/2019 9:14:35 AM","2018-09-12","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Stbd Drain pipe from bridge wing to FAN supply duct,2 angle bars rusted causing rust stains to be cleaned and painted china passage, Stbd side next ER ventilation opening one weld seem to be derusted.","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.4","Very High","","","Derusted and Painted.","2019-06-30","","Completed","2019-06-15","No","No","No","Internal"]
[null,null,null,null,5064,"49_27/10/2019 2:06:31 AM","2018-09-12","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Stbd bridge wing bottom i.e.D deck, derust and pain.","Accommodation","General Appearance","External Factors","11.4","Very High","","","Derusted and Painted.","2019-06-30","","Completed","2019-06-15","No","No","No","Internal"]
[null,null,null,null,4991,"49_25/10/2019 5:21:23 AM","2018-09-18","Defect","Ship Staff","Ship Staff Insp.","IG pressure for 4 P,4 C & 1 S COT showing erroneous reading in CCR. Unable to reset pressure sensor.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.22","Very High","","","Two pressure gauages received at Singaporeon 5th Nov 18. Renewed the defective ones on 4 P & 4 S COT.Currently all cargo showing correct readings.","2018-12-15","NERI180229","Completed","2019-03-06","No","No","No","Internal"]
[null,null,null,null,5005,"49_25/10/2019 7:13:53 AM","2018-10-03","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","MERCATOR name full paintaing on both side hull sides.\t\t\t","Hull & Tanks","General Appearance","External Factors","11.4","Very High","","","Vessel expecting name changed therefore paintaing will be carried out after the changes.","2018-12-30","","Completed","2019-04-01","No","No","No","Internal"]
[null,null,null,null,5017,"49_25/10/2019 8:21:34 AM","2018-10-10","Defect","Ship Staff","Ship Staff Insp.","No 5 S COT PV valve leaking from pressure side.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.22","Very High","","","Overhauled twice. Still leaking. Need spare disc & as the present disc & seat are found with deep pits & highly corroded.","2018-12-30","NERI180260","Completed","2019-04-20","No","No","No","Internal"]
[null,null,null,null,5088,"49_27/10/2019 4:48:14 AM","2018-10-24","Defect","Ship Staff","Ship Staff Insp.","No. 2 COP AUS tank level transimtter requires calibration.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.22","Very High","","","Calibration carried out.","2019-08-15","","Completed","2019-06-20","No","No","No","Internal"]
[null,null,null,null,5089,"49_27/10/2019 4:51:55 AM","2018-11-14","Defect","Ship Staff","Ship Staff Insp.","Cargo educator discharge pressure transmitter defective.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.22","Very High","","","Line cleared, rectified.","2019-08-15","","Completed","2019-06-20","No","No","No","Internal"]
[null,null,null,null,5090,"49_27/10/2019 5:09:10 AM","2018-11-14","Defect","Ship Staff","Ship Staff Insp.","No.3 COP discharged pressure pneumatic transmitter in PR defective.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.22","Very High","","","Line cleared,rectified","2019-08-15","","Completed","2019-06-20","No","No","No","Internal"]
[null,null,null,null,4992,"49_25/10/2019 5:29:28 AM","2018-11-22","Defect","Ship Staff","Ship Staff Insp.","5 P COT PV valve leaking from suction side.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.44","High","","","Lapping and cleaningof seat carried out, No leak observed.","2018-12-15","NERI180260","Completed","2019-03-17","No","No","No","Internal"]
[null,null,null,null,5010,"49_25/10/2019 7:58:35 AM","2018-11-26","Defect","Ship Staff","Ship Staff Insp.","Rudder angle indicator feedback linkage broken.","Hull & Tanks","Navigation","Equipment Related","4.27","High","","","same been welded and fixed,raised req for new one.","2019-01-15","NERI180300","Completed","2019-04-18","No","No","No","Internal"]
[null,null,null,null,5091,"49_27/10/2019 5:13:12 AM","2018-11-30","Defect","Ship Staff","Ship Staff Insp.","No.1 COP discharge & suction local pressure gauge in PR defective.It was compared during line pressure testing.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.22","Very High","","","Line cleared,rectified.","2019-08-15","","Completed","2019-06-20","No","No","No","Internal"]
[null,null,null,null,4967,"49_25/10/2019 2:09:14 AM","2018-12-11","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Snapback zone fwd and aft were not clearly visible due to recently painted deck.# Old snapback zone (sector shaped marking) to.","Hull & Tanks","General Appearance","Knowledge Based","11.4","Very High","","","Old snapback zone removed.","2019-03-31","","Completed","2019-01-19","No","No","No","Internal"]
[null,null,null,null,4995,"49_25/10/2019 6:26:26 AM","2018-12-11","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Vessel does not have any operational microwave in crew or officers pantry","Elect. Mach. & Equip.","MLC Related","Equipment Related","11.13","Low","","","Vessel received 1 microwave during Singapore transit","2019-03-31","","Completed","2019-03-02","No","No","No","Internal"]
[null,null,null,null,5011,"49_25/10/2019 8:04:37 AM","2018-12-11","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Rudder angle indicator in wheel house displays 2 Deg PORT while rudder is midship. The error varies on port and starboard helm.Rudder angle indicator in wheel house displays 2 Deg PORT while rudder is midship. The error varies on port and starboard helm.","Navigation - Others","Navigation","Equipment Related","4.27","High","","","Awaiting spares.","2019-03-31","NERI190014 and NERI190015","Completed","2019-04-18","No","No","No","Internal"]
[null,null,null,null,5012,"49_25/10/2019 8:07:21 AM","2018-12-11","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Transparent acrylic guard on engine lathe machine was found broken","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.12","Very High","","","Face shield kept near the lathe for use","2019-03-31","","Completed","2019-04-18","No","No","No","Internal"]
[null,null,null,null,5048,"49_26/10/2019 6:27:13 AM","2018-12-11","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Removed after installation of new (Wartsila) O2 analyser.","Inert Gas","Eng. / Strg. Comp.","Equipment Related","10.12","Very High","","","Removed.","2019-03-31","","Completed","2019-05-19","No","No","No","Internal"]
[null,null,null,null,5049,"49_26/10/2019 6:36:22 AM","2018-12-11","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Was noticed when foam pump in standby mode.","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.7","Medium","","","Rectified.","2019-03-31","","Completed","2019-05-25","No","No","No","Internal"]
[null,null,null,null,5050,"49_26/10/2019 6:40:51 AM","2018-12-11","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","AUS (Auto unloading system )in CCR is not operational.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.32","Low","","","Troubleshoouting carried out, AUTOMATION to be checked, rectified.","2019-07-31","","Completed","2019-05-18","No","No","No","Internal"]
[null,null,null,null,5069,"49_27/10/2019 2:42:06 AM","2018-12-11","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","No. 1 COP leakage from bottom seal.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.22","Very High","","","Bottom seal renewed.","2019-06-30","","Completed","2019-06-05","No","No","No","Internal"]
[null,null,null,null,5092,"49_27/10/2019 5:19:24 AM","2018-12-11","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Following pressure gauge were found erratic.a) No.3 COP Discharge local and CCR panel gauge, b) Cargo eductor discharge gauge, c) No. 1 COP Suction & discharge gauge(Local).","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.22","Very High","","","Line cleared, rectified.","2019-08-15","","Completed","2019-06-20","No","No","No","Internal"]
[null,null,null,null,5113,"49_27/10/2019 1:01:45 PM","2018-12-11","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Side) located in China passage was found broken.","Hull & Tanks","Structural Condn. / WT integrity ","Equipment Related","11.12","Low","","","Bracket renewed","2019-08-30","","Completed","2019-08-05","No","No","No","Internal"]
[null,null,null,null,4968,"49_25/10/2019 2:12:49 AM","2018-12-15","Defect","Ship Staff","Ship Staff Insp.","Main Engine Unit #7 - FWD Fuel oil high pressure pipe found leaking from the union. Same to be replaced","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.28","Low","","","HP pipe replaced with spare new pipe with adjusted distances as per maker's instructions","2018-12-18","","Completed","2019-12-18","No","No","No","Internal"]
[null,null,null,null,4969,"49_25/10/2019 2:18:00 AM","2019-01-05","Defect","Ship Staff","Ship Staff Insp.","EGE feed pump no.1 - found the FW inlet valve was not operational. Valve spindle found to be broken and valve seat stuck in the body.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.12","Very High","","","Valve replaced with new valve.","2019-01-18","","Completed","2019-01-15","No","No","No","Internal"]
[null,null,null,null,4963,"49_23/10/2019 4:30:46 AM","2019-01-07","Defect","Ship Staff","Ship Staff Insp.","Main drain line of winch hydraulic system is holed.","Deck - Mooring Machinery","Mooring","Equipment Related","9.17","High","","","Hole repaired.","2019-01-15","","Completed","2019-01-10","No","No","No","Internal"]
[null,null,null,null,4965,"49_25/10/2019 1:51:42 AM","2019-01-08","Defect","Ship Staff","Ship Staff Insp.","Locking arrangement for toggle pin of harbour pin is broken.\t","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.29","High","","","Locking arrangement fabricated.","2019-01-10","","Completed","2019-01-09","No","No","No","Internal"]
[null,null,null,null,4970,"49_25/10/2019 2:22:47 AM","2019-01-10","Defect","Ship Staff","Ship Staff Insp.","Tank level float/bob of Waste Oil service tank no:2 was found defective","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.1","Medium","","","Level gauge pulley wire was found stuck and same rectified. Made operational now","2019-01-16","","Completed","2019-01-15","No","No","No","Internal"]
[null,null,null,null,4964,"49_25/10/2019 1:46:40 AM","2019-01-11","Defect","Ship Staff","Ship Staff Insp.","Fresh water tanks vent head mess screen and their frames found in bad condition.","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","Equipment Related","","","","","Mess screen renewed and frames fabricated.","2019-01-14","","Completed","2019-01-11","No","No","No","Internal"]
[null,null,null,null,4971,"49_25/10/2019 2:26:19 AM","2019-01-15","Defect","Ship Staff","Ship Staff Insp.","Steam leaks on purifier heater seam inlet valves and boiler heating return lines to be rectified.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.22","Low","","","Steam leaks attended and rectified.","2019-01-28","","Completed","2019-01-26","No","No","No","Internal"]
[null,null,null,null,4972,"49_25/10/2019 2:29:16 AM","2019-01-17","Defect","Ship Staff","Ship Staff Insp.","Hydrophore tank save all drain line found choked. Same to be cleared.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Pipeline removed and choke rectified. Metal mesh fabricated and put in place.","2019-01-19","","Completed","2019-01-18","No","No","No","Internal"]
[null,null,null,null,5060,"49_26/10/2019 8:32:25 AM","2019-01-24","Defect","Ship Staff","Ship Staff Insp.","Aft motor of port windlass is leakinf from shaft seal.","Deck - Mooring Machinery","Mooring","Equipment Related","9.1","Low","","","Tested, Found no leak. Shall observe during next operation.","2019-04-30","","Completed","2019-04-30","No","No","No","Internal"]
[null,null,null,null,4975,"49_25/10/2019 2:39:12 AM","2019-01-25","Defect","Ship Staff","Ship Staff Insp.","AC blower unit drain line modification to be made","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.8","Medium","","","Drain line cleared and line modified for ease of draining.","2019-02-28","","Completed","2019-02-06","No","No","No","Internal"]
[null,null,null,null,4976,"49_25/10/2019 2:41:29 AM","2019-01-25","Defect","Ship Staff","Ship Staff Insp.","Waste oil service tanks no:1 and 2- vent head flame arrestors to be checked and cleaned.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.23","Medium","","","Same checked and found normal","2019-02-15","","Completed","2019-02-07","No","No","No","Internal"]
[null,null,null,null,4977,"49_25/10/2019 2:43:42 AM","2019-01-28","Defect","Ship Staff","Ship Staff Insp.","Air regulator for control air found defective and not operational","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.34","High","","","Air Regulator isolated and removed from place, Overhauled and put back. Same put in use now.","2019-02-15","","Completed","2019-02-06","No","No","No","Internal"]
[null,null,null,null,4978,"49_25/10/2019 2:49:16 AM","2019-01-30","Defect","Ship Staff","Ship Staff Insp.","ME Fuel Injector Testing machine found to be working inefficiently. Venting function and pressure tsting is found erratic.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.23","Medium","","","Fuel Injector testing machine overhauled with the spares available onboard and same made operational.","2019-02-15","","Completed","2019-02-05","No","No","No","Internal"]
[null,null,null,null,4979,"49_25/10/2019 2:52:10 AM","2019-01-31","Defect","Ship Staff","Ship Staff Insp.","Drinking water hydrophore pump - Gland to be renewed and pump to be overhauled if necessary.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.18","High","","","Pump overhauled and gland packing renewed. Pump operational now.","2019-02-15","","Completed","2019-02-05","No","No","No","Internal"]
[null,null,null,null,4973,"49_25/10/2019 2:32:41 AM","2019-02-07","Defect","Ship Staff","Ship Staff Insp.","A few strands of fwd and aft lashing wire of port life boat were found broken.","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.27","Medium","","","Lashing wire renewed.","2019-02-15","","Completed","2019-02-09","No","No","No","Internal"]
[null,null,null,null,8476,"49_20/12/2019 8:28:55 AM","2019-02-12","Defect","Ship Staff","Nav Audit / Verification","Astronomical sights not being practised regularly.","Navigation - Others","Navigation","Human Error","","","","","All deck officers were instructed to follow company procedures and practice astronomical sights as when weather favours. Sights were practised by all officers and are familiar with use of sextant and calculations.","2019-03-31","","Completed","2019-03-27","No","No","No","Internal"]
[null,null,null,null,4974,"49_25/10/2019 2:36:18 AM","2019-02-12","Defect","Ship Staff","Ship Staff Insp.","Vapour lines drain valves  found choked.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.33","Medium","","","Valves cleared and tried out","2019-02-15","","Completed","2019-02-13","No","No","No","Internal"]
[null,null,null,null,4998,"49_25/10/2019 6:41:45 AM","2019-02-12","Defect","Ship Staff","Ship Staff Insp.","Main Engine units #3 and #6 - Scavenge underpiston temperature high","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.42","Medium","","","During scavenge inspection done on 18/03/2019 found units 3 and 6 top piston rings broken. De-carb of same units carried out on 26/03/2019 and 22/03/2019 respectively.","2019-03-31","","Completed","2019-03-26","No","No","No","Internal"]
[null,null,null,null,4980,"49_25/10/2019 2:54:00 AM","2019-02-14","Defect","Ship Staff","Ship Staff Insp.","Main Engine turbocharger differential pressure manometer for air filter not working. Same to be attended.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.24","Low","","","Manometer removed from place. Cleaned and filled with liquid and fitted back. Same working now.","2019-02-28","","Completed","2019-02-23","No","No","No","Internal"]
[null,null,null,null,4981,"49_25/10/2019 3:00:58 AM","2019-02-16","Defect","Ship Staff","Ship Staff Insp.","Mid-Ships STBD Hose handeling crane- Hydraulic oil leak to be investigated and rectified","Deck - Machinery","Emgcy. Systems","Equipment Related","8.5","Very High","","","Upon investigation, found the seal on Hydraulic oil tank return filter leaking.Same changed with spare new return filter and seal ring.Crane tested found no leaks.","2019-02-28","","Completed","2019-02-22","No","No","No","Internal"]
[null,null,null,null,4997,"49_25/10/2019 6:40:02 AM","2019-02-18","Defect","Ship Staff","Ship Staff Insp.","Railings of the stowing platform of STBD crane jib is broken at 3 places.","Deck - Machinery","General Appearance","Equipment Related","8.5","Very High","","","New railings were fabricated and put in place.","2019-03-31","","Completed","2019-03-18","No","No","No","Internal"]
[null,null,null,null,5013,"49_25/10/2019 8:09:31 AM","2019-02-20","Defect","Ship Staff","Ship Staff Insp.","AE inlet flowmeter not functioning","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.13","Very High","","","Same replaced with new one","2019-04-30","","Completed","2019-04-20","No","No","No","Internal"]
[null,null,null,null,4983,"49_25/10/2019 3:09:00 AM","2019-02-23","Defect","Ship Staff","Ship Staff Insp.","The Auto-drain water separator filter unit fitted on the service air line was found not working","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.19","Very High","","","Unit removed, overhauled and assembled back. Same functional now.","2019-02-28","","Completed","2019-02-25","No","No","No","Internal"]
[null,null,null,null,4985,"49_25/10/2019 3:19:29 AM","2019-02-25","Defect","Ship Staff","Ship Staff Insp.","One of the elbowconnections of hydrualic hoses was found leaking.","Deck - Machinery","General Appearance","Equipment Related","8.47","Very High","","","Leak rectified after braising the connector,crane tried, no leakage observed.","2019-02-27","","Completed","2019-02-27","No","No","No","Internal"]
[null,null,null,null,4984,"49_25/10/2019 3:13:01 AM","2019-02-26","Defect","Ship Staff","Ship Staff Insp.","Aux.Boiler No.1 - One of the heating coil valve flange gasket steam leakage.","E/R - Boiler","Emgcy. Systems","Equipment Related","10.25","Very High","","","Boiler isolated and gasket renewed with meta-flex gasket.","2019-02-26","","Completed","2019-02-26","No","No","No","Internal"]
[null,null,null,null,5125,"49_27/10/2019 1:45:55 PM","2019-02-28","Defect","Ship Staff","Ship Staff Insp.","AE JW cooler 2- SW inlet valve not holding. To be replaced with spare","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.45","Very High","","","Awaiting for anchorage","2019-08-30","","Completed","2019-08-30","No","No","No","Internal"]
[null,null,null,null,5014,"49_25/10/2019 8:12:02 AM","2019-02-28","Defect","Ship Staff","Ship Staff Insp.","....","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","....","2019-04-30","","Completed","2019-04-18","No","No","No","Internal"]
[null,null,null,null,5015,"49_25/10/2019 8:14:09 AM","2019-02-28","Defect","Ship Staff","Ship Staff Insp.","Atmospheric condensor - not coping up. Tubes to be cleaned.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Condenser replaced with spare condenser","2019-04-30","","Completed","2019-04-18","No","No","No","Internal"]
[null,null,null,null,5061,"49_26/10/2019 8:34:24 AM","2019-02-28","Defect","Ship Staff","Ship Staff Insp.","Main Engine- Main air starting valve service limit switch broken and defective","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.12","Very High","","","Repairs carried out.","2019-08-30","","Completed","2019-05-30","No","No","No","Internal"]
[null,null,null,null,5075,"49_27/10/2019 3:28:47 AM","2019-02-28","Defect","Ship Staff","Ship Staff Insp.","Hot well top covers and top plate corroded and leaking","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.14","Medium","","","Top plate de rusted and painted","2019-06-15","","Completed","2019-06-02","No","No","No","Internal"]
[null,null,null,null,4990,"49_25/10/2019 4:41:30 AM","2019-03-06","Defect","Ship Staff","Ship Staff Insp.","Protective rail on STBD crane operator platform found broken and out of place.","Deck - Machinery","Emgcy. Systems","Equipment Related","","","","","A new protective handle fabricated and put in place.","2019-03-15","","Completed","2019-03-10","No","No","No","Internal"]
[null,null,null,null,4993,"49_25/10/2019 5:31:59 AM","2019-03-10","Defect","Ship Staff","Ship Staff Insp.","ME unit #5- HP Fuel pump's FWD high pressure pipe found leaking","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.45","Very High","","","HP pipe replaced with a spare new pipe","2019-03-15","","Completed","2019-03-12","No","No","No","Internal"]
[null,null,null,null,4994,"49_25/10/2019 5:57:55 AM","2019-03-15","Defect","Ship Staff","Ship Staff Insp.","ME #2 unit - Air starting valve found leaking","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.45","Very High","","","Same replace with a sapre overhauled valve","2019-03-20","","Completed","2019-03-16","No","No","No","Internal"]
[null,null,null,null,5002,"49_25/10/2019 6:58:28 AM","2019-03-16","Defect","Ship Staff","Ship Staff Insp.","Mooring winch no3 aft drum's brake handle is found defective.","Deck - Mooring Machinery","Emgcy. Systems","Equipment Related","9.12","Medium","","","Handle removed and locking plate fixed,put in place and tested.","2019-03-19","","Completed","2019-03-18","No","No","No","Internal"]
[null,null,null,null,4999,"49_25/10/2019 6:43:56 AM","2019-03-17","Defect","Ship Staff","Ship Staff Insp.","Air Con. condensor cooling SW return line pipe section leaking","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.15","Low","","","Pipe section removed. Found to be holed. Pipe section fabricated and same renewed","2019-04-15","","Completed","2019-04-02","No","No","No","Internal"]
[null,null,null,null,5000,"49_25/10/2019 6:45:52 AM","2019-03-18","Defect","Ship Staff","Ship Staff Insp.","ME unit #2 - Exhaust valve FW leak from bottom piece O-rings. Same to be renewed.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.24","Low","","","Exhaust valve pulled out and O-rings renewed and no FW leaks now.","2019-04-15","","Completed","2019-03-30","No","No","No","Internal"]
[null,null,null,null,5003,"49_25/10/2019 7:03:20 AM","2019-03-26","Defect","Ship Staff","Ship Staff Insp.","Jib stowing platform of both the hose handling crane does not have protective chains/rails.","Deck - Machinery","Emgcy. Systems","Equipment Related","9.16","High","","","Chain arrangement made to secure the stowing platform.","2019-03-31","","Completed","2019-03-28","No","No","No","Internal"]
[null,null,null,null,5004,"49_25/10/2019 7:07:28 AM","2019-03-28","Defect","Ship Staff","Ship Staff Insp.","Air hose of STBD gangway shifting motor was found defective and leaking.","Deck - Machinery","General Appearance","Equipment Related","11.2","Medium","","","Air hose replaced with the new one.","2019-03-31","","Completed","2019-03-29","No","No","No","Internal"]
[null,null,null,null,5009,"49_25/10/2019 7:53:46 AM","2019-03-28","Defect","Ship Staff","Ship Staff Insp.","Floats of ballast vent heads of 3P Fwd, 3P Aft, 4P Fwd, 4S Aft were found to have slight crack in the body.","Miscellaneous","Cargo / Ballast Systems","Equipment Related","8.22","Very High","","","Replace with new ones.","2019-04-30","NERI190073","Completed","2019-04-11","No","No","No","Internal"]
[null,null,null,null,5008,"49_25/10/2019 7:47:37 AM","2019-03-31","Defect","Ship Staff","Ship Staff Insp.","U- clamps of life buoy's bracket on stbd side aft of the manifold is heavily rusted.","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.28","Very High","","","New U- clamps to be put in place after removing the old ones.","2019-04-07","","Completed","2019-04-02","No","No","No","Internal"]
[null,null,null,null,5148,"49_27/10/2019 4:21:59 PM","2019-04-01","Defect","Ship Staff","Ship Staff Insp.","Boiler feed pumps no2 heavy vibrations and seal leak","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","pump overhauled","2019-08-30","RESP190035","Completed","2019-09-28","No","No","No","Internal"]
[null,null,null,null,5149,"49_27/10/2019 4:25:03 PM","2019-04-01","Defect","Ship Staff","Ship Staff Insp.","Port gangway shifting motor not working.","Deck - Machinery","Emgcy. Systems","Equipment Related","5.33","High","","","Fitted and working satisfactory.","2019-09-10","RESP195075","Completed","2019-09-20","No","No","No","Internal"]
[null,null,null,null,5007,"49_25/10/2019 7:19:18 AM","2019-04-01","Defect","Ship Staff","Ship Staff Insp.","Solenoid operated direction control valve no:40 for VIT actuator found leaking on Main Engine pneumatic control system","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Same replaced with spare new valve and found satisfactory.","2019-04-15","","Completed","2019-04-03","No","No","No","Internal"]
[null,null,null,null,5150,"49_27/10/2019 4:26:26 PM","2019-04-05","Defect","Ship Staff","Ship Staff Insp.","Valve no: 265(V11) - Super Spool Pneumatic Direction valve (Type: PSMT - 33) for puncture valve actuator for each unit found leaking.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.13","Very High","","","Leak rectified","2019-10-15","","Completed","2019-10-19","No","No","No","Internal"]
[null,null,null,null,5151,"49_27/10/2019 4:27:47 PM","2019-04-05","Defect","Ship Staff","Ship Staff Insp.","Reducing valve no: 59 and valve no 45 found leaking on Main Engine Pneumatic control system","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.14","Medium","","","Leaky valve renewed","2019-10-15","","Completed","2019-10-14","No","No","No","Internal"]
[null,null,null,null,5016,"49_25/10/2019 8:15:54 AM","2019-04-05","Defect","Ship Staff","Ship Staff Insp.","Atmospheric condenser steam dumping valves leaks","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.17","Very High","","","Overhauled reducing valve and isolation valve","2019-05-01","","Completed","2019-04-18","No","No","No","Internal"]
[null,null,null,null,8472,"49_20/12/2019 8:10:49 AM","2019-04-16","Defect","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","No evidence showing regulators located at Oxygen & Acetylene cylinders side were inspected annually and replaced/refurbished 5Y basis as per manufacturers instructions","Miscellaneous","General Appearance","Equipment Related","5.26","Medium","","","Regulators inspected and a record generated serving as a proof of the same being done.","2019-05-31","","Completed","2019-05-10","No","No","No","External"]
[null,null,null,null,9985,"49_03/01/2020 8:44:20 PM","2019-04-25","Observation","Owner / Marine / Tech. Suptd.","Nav Audit / Verification","The Log book entry had a few over writtings which were not initialled by the OOW","Miscellaneous","Cert. & Docu.","Human Error","4.2","Medium","","","All OOW were educated regarding the importance of not over writing and to strike with a single line and counter-signing if and when any error is made while filling any official document. The purpose being that the mistake made must be readily apparent to the auditor so that there are no indications of any malpractise. ","2019-04-30","","Completed","2019-04-25","No","No","No","Internal"]
[null,null,null,null,9986,"49_6/1/2020 5:19:57 PM","2019-04-25","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","No.1 manifold port side blank 2 bolts are of smaller length with no threads visible.","Cargo Mach.","Cargo / Ballast Systems","Human Error","8.41","Medium","","","The bolts have been replaced with correct length of bolts. All smaller bolts have been kept separated so that can not be mistaken again.","2019-05-25","","Completed","2019-05-01","No","No","No","Internal"]
[null,null,null,null,9987,"49_6/1/2020 5:24:21 PM","2019-04-25","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","The MSDS posted in CCR was not of present cargo.","Documentation","Cargo / Ballast Systems","Human Error","5.46","Medium","","","MSDS of present cargo onboard has been put immediately. ","2019-04-25","","Completed","2019-04-25","No","No","No","Internal"]
[null,null,null,null,9988,"49_6/1/2020 5:28:28 PM","2019-04-25","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","The pressure gauge of no.1 manifold was showing 9 bars whilw the one of no.2 manifold was showing 8 bars. As crossovers were open and vessel was discharging in a common line it was suspected that one of the pressure gauges had an error.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.8","Medium","","","Defective pressure gauge replaced.","2019-05-25","","Completed","2019-05-01","No","No","No","Internal"]
[null,null,null,null,9989,"49_6/1/2020 5:32:32 PM","2019-04-25","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Valve open indicator light was found fused for 4P WBT.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.8","Medium","","","The defective indicator bulb rectified.","2019-05-01","","Completed","2019-05-01","No","No","No","Internal"]
[null,null,null,null,5126,"49_27/10/2019 1:47:33 PM","2019-04-25","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ME fuel p/p's- all umbrella seals have been reported are leaking. To be investigated","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.25","Very High","","","Investigation carried out foud no seal leak","2019-07-30","","Completed","2019-08-21","No","No","No","Internal"]
[null,null,null,null,9990,"49_6/1/2020 5:39:30 PM","2019-04-25","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","The time of commencement of de-ballasting operation was missing for last loading operation. ","Documentation","Cargo / Ballast Systems","Human Error","8.5","Very High","","","The time of commencement has been entered in the CCR log from SOF.","2019-04-25","","Completed","2019-04-25","No","No","No","Internal"]
[null,null,null,null,5127,"49_27/10/2019 1:49:08 PM","2019-04-25","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","It has been reported by CE that CLO consumption from Alpha lubricator stroke calculations is not matching with actual","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.25","Very High","","","Investigation carried out. Found calculation is matching","2019-08-24","","Completed","2019-08-21","No","No","No","Internal"]
[null,null,null,null,5128,"49_27/10/2019 1:51:02 PM","2019-04-25","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Coverings on ECR chairs are torn. Same to be renewed","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.14","Medium","","","No rexin available on board, item will be added to ER store requisition","2019-07-30","RESP190063","Completed","2019-08-25","No","No","No","Internal"]
[null,null,null,null,5130,"49_27/10/2019 1:58:06 PM","2019-04-25","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","IG automation is not working. Transmitter is on order. To be rectified as soon as spares are received.","Inert Gas","Eng. / Strg. Comp.","Equipment Related","10.12","Very High","","","Transmitter renewed","2019-07-15","","Completed","2019-08-25","No","No","No","Internal"]
[null,null,null,null,5131,"49_27/10/2019 2:01:50 PM","2019-04-25","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Hydraulic pipes connecting the hydraulic motors on mooring winches are in very poor condition. New pipes to be fabricated and renewed.","Deck - Mooring Machinery","Mooring","Equipment Related","10.12","Very High","","","some pipe renewed.","2019-08-30","","Completed","2019-08-20","No","No","No","Internal"]
[null,null,null,null,5132,"49_27/10/2019 2:05:41 PM","2019-04-25","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Gas tight UTI- only ONE more to be supplied.","Miscellaneous","Cargo / Ballast Systems","Equipment Related","8.21","High","","","Awaiting Supply. To be procured directly from office.","2019-08-15","","Completed","2019-08-24","No","No","No","Internal"]
[null,null,null,null,5133,"49_27/10/2019 3:20:25 PM","2019-04-25","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Vessel does not have spare wire for: Hose handling crane, gangway and lifeboat.Same to be.","Deck - Machinery","Mooring","Equipment Related","","","","","Recevied in Singapore.","2019-08-15","RESP195062","Completed","2019-08-23","No","No","No","Internal"]
[null,null,null,null,9998,"49_20-Jan-20 8:10:46 PM","2019-04-25","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","PMS reporting not found proper. Some monthly forms were not found attached with the reported jobs. Same to be corrected as discussed in detail with C/E and 2/E. History books to be regularly updated.","Documentation","Cert. & Docu.","Equipment Related","2.12","Low","","","Same discussed","2019-05-10","","Completed","2019-04-27","No","No","No","Internal"]
[null,null,null,null,9999,"49_20-Jan-20 8:14:36 PM","2019-04-25","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Windlass stbd motor leakages to attend, leakages found in both motors and handle","Deck - Mooring Machinery","Mooring","Equipment Related","","","","","Motor shaft seal renewed","2019-06-25","","Completed","2019-07-18","No","No","No","Internal"]
[null,null,null,null,10000,"49_20-Jan-20 8:19:37 PM","2019-04-25","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Windlass port motor leakages aft to attend","Deck - Mooring Machinery","Mooring","Equipment Related","9.1","Low","","","Motor shaft seal renewed","2019-06-25","","Completed","2019-07-29","No","No","No","Internal"]
[null,null,null,null,10001,"49_20-Jan-20 8:22:58 PM","2019-04-25","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Foam p/p trial is a critical job and cannot be postponed, additionally there is leakage in the pump gland, to be rectified","Deck - Machinery,LSA / FFA","Safety / LSA / FFA","Equipment Related","5.12","Medium","","","Same rectified","2019-05-10","","Completed","2019-04-29","No","No","No","Internal"]
[null,null,null,null,10002,"49_20-Jan-20 8:27:08 PM","2019-04-25","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","CO2 room and steering gear mushroom vent to de-rust and vents to be rectified","E/R - Aux. Mach.,LSA / FFA","Eng. / Strg. Comp.","Equipment Related","","","","","Same rectified","2019-05-10","","Completed","2019-05-03","No","No","No","Internal"]
[null,null,null,null,10003,"49_20-Jan-20 8:29:53 PM","2019-04-25","Defect,Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Emergency Fire pump mechanical seal and leakages to rectify","LSA / FFA","Eng. / Strg. Comp.","Equipment Related","5.38","High","","","Same rectified","2019-05-10","","Completed","2019-05-02","No","No","No","Internal"]
[null,null,null,null,10004,"49_20-Jan-20 8:32:06 PM","2019-04-25","Defect,Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","WS lathe mc should fabricate transparent safety shied to avoid injury to eye of personnel carrying the job(recommended).","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Same rectified","2019-05-10","","Completed","2019-08-29","No","No","No","Internal"]
[null,null,null,null,10005,"49_20-Jan-20 8:34:34 PM","2019-04-25","Defect,Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Fwd ME  air cooler sw inlet pipe leaking.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.13","Very High","","","Rectified","2019-05-25","","Completed","2019-05-25","No","No","No","Internal"]
[null,null,null,null,10006,"49_20-Jan-20 8:42:10 PM","2019-04-25","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Audible alarm for the IG pressure in CCR hooter not operational in CCR but operational in Bridge ","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.42","Medium","","","Same rectified","2019-05-25","","Completed","2019-05-25","No","No","No","Internal"]
[null,null,null,null,10007,"49_20-Jan-20 8:45:49 PM","2019-04-25","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ME LO purifier should be operational 24X7 , found not operational during the ship visit ","E/R - Aux. Mach.","Eng. / Strg. Comp.","Inappropriate Procedure","10.27","Medium","","","Same instruction followed","2019-05-10","","Completed","2019-04-26","No","No","No","Internal"]
[null,null,null,null,10008,"49_20-Jan-20 8:48:30 PM","2019-04-25","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Doctor , Performance  report export (.ilb file )to be submitted for the Vessel for each month , not received for the past few months ","Miscellaneous","Cert. & Docu.","Human Error","","","","","Same instruction followed","2019-05-02","","Completed","2019-04-26","No","No","No","Internal"]
[null,null,null,null,10009,"49_20-Jan-20 8:50:33 PM","2019-04-25","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","EGE feed Pump no.1 vibration and leakages need to attend ","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","8.25","Very High","","","Seal renewed","2019-05-10","","Completed","2019-04-30","No","No","No","Internal"]
[null,null,null,null,10010,"49_20-Jan-20 8:52:01 PM","2019-04-25","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","EGE feed pump No.2 found no leakages at low load during visit, all impellers renewed \n\nLast Ce updated leakages in Mechanical seal , spares onboard \n\n","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","8.25","Very High","","","Seal renewed","2019-05-10","","Completed","2019-04-29","No","No","No","Internal"]
[null,null,null,null,10011,"49_20-Jan-20 8:54:22 PM","2019-04-25","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Engine room vent fan , derusting and painting of the rooms and Fan casings to be carried out ","E/R - Aux. Mach.","General Appearance","Equipment Related","8.12","Medium","","","Same carried out","2019-05-10","","Completed","2019-04-28","No","No","No","Internal"]
[null,null,null,null,10012,"49_20-Jan-20 8:57:19 PM","2019-04-25","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Port side bunker high level alarm electrical pipe support bar wasted, needs renewal.","E/R - Pipes/ valves & fittings","General Appearance","Equipment Related","11.4","Very High","","","Same rectified","2019-05-10","","Completed","2019-05-02","No","No","No","Internal"]
[null,null,null,null,10013,"49_20-Jan-20 8:59:02 PM","2019-04-25","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Electrical wire support bar for emg lightening near LB launching procedures wasted, needs renewal.","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.1","High","","","Same rectified","2019-05-10","","Completed","2019-05-02","No","No","No","Internal"]
[null,null,null,null,10014,"49_20-Jan-20 8:38:45 PM","2019-04-25","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Notice near 15 ppm should mentioned “not to be operated without permission of Master & CE”.Presently only mentioned CE ","Miscellaneous","Cert. & Docu.","Equipment Related,Human Error","","","","","Notice put in place","2019-04-28","","Completed","2019-04-25","No","No","No","Internal"]
[null,null,null,null,10015,"49_20-Jan-20 9:00:22 PM","2019-04-25","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","STBD side conduit pipe near LB ,electrical wire pocket needs to be filled with electrical putty ","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.1","High","","","Same rectified","2019-05-10","","Completed","2019-05-02","No","No","No","Internal"]
[null,null,null,null,5152,"49_27/10/2019 4:30:44 PM","2019-04-25","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Manoeuvring system VIT valves require overhauling. Kits are on order same to be renewed","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.24","Low","","","Leaky valves renewed","2019-10-15","","Completed","2019-10-14","No","No","No","Internal"]
[null,null,null,null,10016,"49_20-Jan-20 9:02:54 PM","2019-04-25","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Galley- Dishwasher not working. To be repaired or new one to be procured.","Accommodation ","General Appearance","Equipment Related","11.5","Medium","","","Same rectified","2019-05-25","","Completed","2019-05-12","No","No","No","Internal"]
[null,null,null,null,10017,"49_20-Jan-20 9:04:39 PM","2019-04-25","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Galley- Fridge not working. To be repaired or new one to be procured.","Accommodation ","General Appearance","Equipment Related","11.5","Medium","","","Same rectified, working","2019-05-25","","Completed","2019-05-08","No","No","No","Internal"]
[null,null,null,null,10018,"49_21/01/2020 5:28:47 AM","2019-04-25","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Chequckered plates of ramps are in poor condition. These to be dismantled or cut and fabricated. To be fixed back by bolted arrange","Miscellaneous","General Appearance","External Factors","11.3","Medium","","","Completed.","2019-07-24","","Completed","2019-07-23","No","No","No","Internal"]
[null,null,null,null,10019,"49_21/01/2020 5:54:35 AM","2019-04-25","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Port side crane jib pins locking bolt is bent. Same to be made free..","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.63","High","","","Made free.","2019-07-24","","Completed","2019-07-10","No","No","No","Internal"]
[null,null,null,null,5157,"49_27/10/2019 4:45:25 PM","2019-04-25","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Ladder step on the mainfold are in poor condition.These are to be repaired.","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.1","High","","","Both PORT & STBD manifolds de- rusted and painted including ladders.","2019-10-30","","Completed","2019-10-13","No","No","No","Internal"]
[null,null,null,null,4921,"49_24/10/2019 3:58:43 AM","2019-04-25","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Cover of gears for all winches and windlass are in poor condition.Covers to be removed repaired and reinstalled after blasting and painting two coats of epoxy paint.","Deck - Mooring Machinery","Mooring","Equipment Related","9.14","Medium","","","All winches damaged cover gears removed and fitted back. Only windlass gear covers remaining. Job planned after completion of fwd mooring area grit blasting.","2020-03-15","","Completed","2020-11-21","No","No","No","Internal","Target date already over due.  Pls revert with update on progress status & a realistic target date."]
[null,null,null,null,4922,"49_24/10/2019 4:48:41 AM","2019-04-25","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Windlass and all winches to be fully blast and repaint with two coats of primer and one final coat red colour (same as deck colour) paint.","Deck - Mooring Machinery","","Equipment Related","9.14","Medium","","","De-rusting of poop deck mooring winches and 2 coats of primer & final coat completed.","2020-03-20","RESP190062","Completed","2020-11-21","No","No","No","Internal","Pls update progress status for the remaining winches & indicate a realistic target date, as the existing target date is already overrun by approx. 8 months."]
[null,null,null,null,4925,"49_24/10/2019 5:55:15 PM","2019-04-25","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Galley-Fridge not working. To be repaired or new one one to be procured.","Miscellaneous","MLC Related","Equipment Related","11.16","Low","","","Received new fridge for galley, same installed, securing arrangement made and put in to use.","2020-08-20","RESP200185","Completed","2020-09-07","No","No","No","Internal","Please update status on progress of installation & indicate a realistic target date."]
[null,null,null,null,4926,"49_24/10/2019 6:01:44 PM","2019-04-25","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Mooring Tails usage hrs have exceeded 18 months. To be replaced during next storing.","Miscellaneous","Mooring","Equipment Related","9.17","High","","","Received 20 new mooring tails 25 Jan 2020 at Singapore. Same renewed and updated in mooring matrix. Old tails offlanded at Singapore","2020-01-31","RESP195064","Completed","2020-01-31","No","No","No","Internal",""]
[null,null,null,null,4939,"49_25/10/2019 7:21:58 PM","2019-04-25","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Before start of manoeuvring, after the engine is blow through, duty engineer to log in the E/R control log that the engine movements are given as per telegraph logger","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Clear instruction given to duty engineer to log in the E/R Control log that the engine movements are given as per telegraph","2019-04-29","","Completed","2019-04-25","No","No","No","Internal"]
[null,null,null,null,4940,"49_25/10/2019 7:23:43 PM","2019-04-25","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Temp control xv/v for Pfr is leaking. To be rectified","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.23","Medium","","","Temp control xv/v for Pfr gland tightened and leak recified","2019-06-23","","Completed","2019-04-26","No","No","No","Internal"]
[null,null,null,null,4941,"49_25/10/2019 7:29:41 PM","2019-04-25","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Both vacuum pumps for Fire and Bilge p/p's, Vacuum p/p are seized.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.21","Medium","","","Vacuum pump overhauled. Its in operation.","2019-06-01","","Completed","2019-06-01","No","No","No","Internal"]
[null,null,null,null,4942,"49_25/10/2019 7:31:48 PM","2019-04-25","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","The main air bottle auto drain valve was found shut. To be overhauled and put back in operation","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Auto drain valve overhauled, put back in operation.","2019-05-11","","Completed","2019-07-02","No","No","No","Internal"]
[null,null,null,null,4943,"49_25/10/2019 7:42:49 PM","2019-04-25","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","The door closer of Funnel door is defective. To be repaired.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","The door closer of Funnel door is repaired.","2019-05-11","","Completed","2019-05-10","No","No","No","Internal"]
[null,null,null,null,4944,"49_25/10/2019 7:44:26 PM","2019-04-25","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Electric starter panels are dirty, all of them are to be cleaned","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.28","Low","","","Electric starter panels are cleaned.","2019-07-23","","Completed","2019-05-05","No","No","No","Internal"]
[null,null,null,null,4945,"49_25/10/2019 7:46:16 PM","2019-04-25","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Some lights were found not working in E/R casing. To be replaced.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Lights were renewed.","2019-05-24","","Completed","2019-04-26","No","No","No","Internal"]
[null,null,null,null,4946,"49_25/10/2019 7:48:07 PM","2019-04-25","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Hot water leak on 3rd deck. To be rectified.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.47","Medium","","","Leak rectified.","2019-06-23","","Completed","2019-05-25","No","No","No","Internal"]
[null,null,null,null,5021,"49_25/10/2019 9:01:20 AM","2019-04-25","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Some of the mesh for Ballast tank vent were found with incorrect size. All mesh to be checked and the ones which are big in size are to be replaced with correct size mesh.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.4","Medium","","","All Ballast vent mesh renewed.","2019-05-05","","Completed","2019-04-26","No","No","No","Internal"]
[null,null,null,null,5022,"49_25/10/2019 5:33:38 PM","2019-04-25","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Some of the mesh for ballast tank ventwere found with incorrect size.All mesh to be checked and one which are big in size are to be replaced with correct size mesh.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.4","Medium","","","All ballast vents mesh renewed.","2019-05-05","","Completed","2019-04-26","No","No","No","Internal"]
[null,null,null,null,5030,"49_25/10/2019 6:18:58 PM","2019-04-25","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","COW machines to be de-rusted and painted.","Cargo Mach.","General Appearance","Equipment Related","8.56","Medium","","","COW machine valves greased and freed.","2019-05-20","","Completed","2019-05-18","No","No","No","Internal"]
[null,null,null,null,5031,"49_25/10/2019 6:22:41 PM","2019-04-25","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","All areas where primer has been applied to be washed and repainted at the earliest as recoating interval is only 15 days.","Hull & Tanks","General Appearance","Inappropriate Procedure","11.2","Medium","","","All primered areas throughly washed and painted.","2019-05-20","","Completed","2019-05-20","No","No","No","Internal"]
[null,null,null,null,5033,"49_25/10/2019 6:28:39 PM","2019-04-25","Defect","Ship Staff","Ship Staff Insp.","No.2S COT PV valve leaking from pressure side.","Inert Gas","Cargo / Ballast Systems","Equipment Related","8.39","Medium","","","Overhauled, lapped the pressure seat and rectified.","2019-07-25","NERI190091","Completed","2019-05-21","No","No","No","Internal"]
[null,null,null,null,5034,"49_25/10/2019 6:43:20 PM","2019-04-25","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","COW line and fire line valves on deck found frozen. All these valves to be made free.","Deck - Machinery","Cargo / Ballast Systems","Equipment Related","8.45","High","","","All COW and fire line valves made free, operable by hande.","2019-05-19","","Completed","2019-05-19","No","No","No","Internal"]
[null,null,null,null,5051,"49_26/10/2019 6:45:24 AM","2019-04-25","Defect","Ship Staff","Ship Staff Insp.","No 1 GPS stoped responding and not showing dispaly after replacement of internal battery by service engineer during annual at Qinhuangdao.","Navigation - DGPS / EPFS / AIS","Navigation","Equipment Related","4.27","High","","","New unit installed in Singapore,on 6th may 2019.","2019-05-08","","Completed","2019-05-06","No","No","No","Internal"]
[null,null,null,null,5052,"49_26/10/2019 6:49:44 AM","2019-04-25","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Hydro blaster motor is in poor condition.Maintenance to be carried out on the same and stored properly and properly covering with conwase.","Hull & Tanks","Structural Condn. / WT integrity ","Equipment Related","","","","","Maintenance carried out.","2019-05-20","","Completed","2019-05-18","No","No","No","Internal"]
[null,null,null,null,5053,"49_26/10/2019 6:59:51 AM","2019-04-25","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Galley - Potato peeler not working.To be repaired.","Miscellaneous","MLC Related","Equipment Related","","","","","Repaired.","2019-05-20","","Completed","2019-05-15","No","No","No","Internal"]
[null,null,null,null,5054,"49_26/10/2019 7:03:58 AM","2019-04-25","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Galley- Mixer not woking.To be repaired.","Miscellaneous","General Appearance","Equipment Related","","","","","Repaired.","2019-05-20","","Completed","2019-05-15","No","No","No","Internal"]
[null,null,null,null,5055,"49_26/10/2019 7:10:25 AM","2019-04-25","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Condition of cabin toilate to be improved.Many shower have been found leaking.Same to be rectified/renewed as necessary. Some flush in crew cabin has been reported as not working. Same to be rectified.","Accommodation","MLC Related","Equipment Related","11.3","Medium","","","Cleaning carried out.Leaking shower head replaced.","2019-06-15","","Completed","2019-05-15","No","No","No","Internal"]
[null,null,null,null,5056,"49_25/10/2019 7:12:22 PM","2019-04-25","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Mattresses in some cabins are in poor condition. same to renewed.","Accommodation","General Appearance","Human Error","11.3","Medium","","","Mattresses renewed.","2019-07-30","","Completed","2019-05-28","No","No","No","Internal"]
[null,null,null,null,5058,"49_26/10/2019 7:27:15 AM","2019-04-25","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Boiler feed pump No.1 has been reported to be in poor condition.Spares to be supplied and same to.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","8.41","Medium","","","Wating for spare.","2019-06-23","RESP195028","Completed","2019-05-28","No","No","No","Internal"]
[null,null,null,null,5059,"49_26/10/2019 7:30:07 AM","2019-04-25","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","AE LO attached p/p'sdue for overhaul. Spares to be ordered and pumps overhauled","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","8.24","Medium","","","Waiting for spare","2019-06-23","NERI190033","Completed","2019-05-20","No","No","No","Internal"]
[null,null,null,null,5062,"49_26/10/2019 8:40:56 AM","2019-04-25","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Leak on port windlass motor shaft seal.Seal to renew. Job to be undertaken in the ballast.","Deck - Mooring Machinery","Mooring","Equipment Related","9.25","Low","","","Tested.Found no leak.Shall observe during next ops.","2019-05-30","","Completed","2019-05-30","No","No","No","Internal"]
[null,null,null,null,5065,"49_27/10/2019 2:10:56 AM","2019-04-25","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","AUS not working.To be recalibrated.Water was found in control system.Efficiency of control air dryer to be checked.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.37","High","","","AUS automation and valve operations repaired and tried out.","2019-05-20","","Completed","2019-05-18","No","No","No","Internal"]
[null,null,null,null,5070,"49_27/10/2019 2:48:41 AM","2019-04-25","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Galley- A/C not working. To be repaired. Spares to be ordered.","Miscellaneous","MLC Related","Equipment Related","11.3","Medium","","","Repaired working fine.","2019-06-20","","Completed","2019-06-14","No","No","No","Internal"]
[null,null,null,null,5084,"49_27/10/2019 4:11:27 AM","2019-04-25","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Cargo Pressure monitoring system alarms in CCR is not working. To be rectified.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.41","Medium","","","Cargo pressur monitoring system in CCR checked,Alarm module is inactive in softwear, Unable to activate by ship staff.","2019-08-20","","Completed","2019-06-16","No","No","No","Internal"]
[null,null,null,null,5085,"49_27/10/2019 4:13:39 AM","2019-04-25","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","AC for the MSB room is not working. To be repaired on priority","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.13","Very High","","","Repaired carried out. Working satisfactorily","2019-07-25","","Completed","2019-06-16","No","No","No","Internal"]
[null,null,null,null,5093,"49_27/10/2019 5:24:08 AM","2019-04-25","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","In many areas old paint is peeling off on main deck.These section to be blasted and repainted.Vessel to start using the girt blaster and hydro.","Hull & Tanks","General Appearance","Equipment Related","11.3","Medium","","","Hydroblasting completed.","2019-06-25","","Completed","2019-06-18","No","No","No","Internal"]
[null,null,null,null,5094,"49_27/10/2019 5:30:25 AM","2019-04-25","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Rusted area below the pipeline to be attended.This job to be put on priority now.Area to be blasted and coated with two coats of primer and one coat of polyurthane paint.","Hull & Tanks","General Appearance","Equipment Related","11.3","Medium","","","Hydroblasting completed.","2019-06-25","","Completed","2019-06-18","No","No","No","Internal"]
[null,null,null,null,5102,"49_27/10/2019 6:40:38 AM","2019-04-25","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Engine casing area is dirty - To be cleaned","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.1","Medium","","","Cleaning and Painting done","2019-08-30","","Completed","2019-07-16","No","No","No","Internal"]
[null,null,null,null,5103,"49_27/10/2019 6:45:48 AM","2019-04-25","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Port side crane control block pipe/ connectors are to be renewed as in poor condition.","Deck - Machinery","Structural Condn. / WT integrity ","Equipment Related","9.25","Low","","","Inspection carried out, connectors cleaned , no leaky from connectors.","2019-07-30","","Completed","2019-07-17","No","No","No","Internal"]
[null,null,null,null,5111,"49_27/10/2019 12:56:53 PM","2019-04-25","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Winch 4,7 wire end securing hook bent.To be repaired.","Deck - Mooring Machinery","Mooring","Equipment Related","9.12","Medium","","","Repaired.","2019-07-25","","Completed","2019-07-25","No","No","No","Internal"]
[null,null,null,null,5112,"49_27/10/2019 12:58:28 PM","2019-04-25","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Valves for AC condensers, Steam condensers and Boiler water circulation P/P outlet to No.1 are not holding. Same to be repaired/renewed","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Valves for AC condenser remaining","2019-07-30","","Completed","2019-07-31","No","No","No","Internal"]
[null,null,null,null,5118,"49_27/10/2019 1:17:41 PM","2019-04-25","Defect","Ship Staff","Suptd. Insp.","Mesh of pump room blower are in poor condition.Mesh to removed, the frame from inside to chipped and painted and new mesh is to installed.","Hull & Tanks","General Appearance","Equipment Related","11.1","High","","","Pumproom blower complete derusting. Two coats primer and final coat carried out.","2019-08-30","","Completed","2019-08-10","No","No","No","Internal"]
[null,null,null,null,5119,"49_27/10/2019 1:24:59 PM","2019-04-25","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Hydraulic boxes forward to be blasted and painted red. The boxes are also to be derusted and painted from the bottam as it was seen on the boxes where blasting has been done the bottom...................... ","Miscellaneous","General Appearance","Equipment Related","11.1","High","","","All hydraulic boxes on deck completed derusting two coats primer and final coat.","2019-08-12","","Completed","2019-08-09","No","No","No","Internal"]
[null,null,null,null,5045,"49_26/10/2019 6:03:07 AM","2019-05-01","Defect","Ship Staff","Ship Staff Insp.","Fuel oil auto backwash filter elemens choked cannot be cleaned. Auto backwash filter not in use","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.24","Low","","","New elements put in use, fuel oil backwash filter working.","2019-05-01","","Completed","2019-05-10","No","No","No","Internal"]
[null,null,null,null,8473,"49_20/12/2019 8:16:07 AM","2019-05-07","Defect","PSC Insp.","PSC Inspection","Three E/R dampers when in closed position found gaps of atleast 3mm at intervals, thus unable to provide effective isolation during emergency","Miscellaneous","Emgcy. Systems","Equipment Related","5.35","Medium","Fire safety","","Dampers repaired, operation tested and sighted by Class inspector. Found in good working condition.","2019-05-07","","Completed","2019-05-07","No","No","No","External"]
[null,null,null,null,8474,"49_20/12/2019 8:19:43 AM","2019-05-07","Defect","PSC Insp.","PSC Inspection","Emergency generator DO tank air vent found severely corroded and hole.","Critical Equip.","Emgcy. Systems","Equipment Related","11.7","High","Fire safety","","Air vent repaired and verified by Class inspector.","2019-05-07","","Completed","2019-05-07","No","No","No","External"]
[null,null,null,null,4947,"49_25/10/2019 7:50:49 PM","2019-05-07","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Hydrophore pump leaking","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.47","Medium","","","Gland packing tightened leak rectified","2019-06-20","","Completed","2019-06-08","No","No","No","Internal"]
[null,null,null,null,4948,"49_25/10/2019 7:52:23 PM","2019-05-07","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Emergency air bottle pressure was zero","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.47","Medium","","","Emergency air bottle filled and kept as standby","2019-05-20","","Completed","2019-05-09","No","No","No","Internal"]
[null,null,null,null,4949,"49_25/10/2019 7:58:38 PM","2019-05-07","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Jacket cooler SW pipe leaking","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.47","Medium","","","Jacket cooler SW pipe renewed","2019-05-31","","Completed","2019-05-23","No","No","No","Internal"]
[null,null,null,null,4950,"49_25/10/2019 8:00:07 PM","2019-05-07","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","....","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","....","2019-05-31","","Completed","2019-05-23","No","No","No","Internal"]
[null,null,null,null,5023,"49_25/10/2019 5:37:33 PM","2019-05-07","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ODME printer cartridge needs to be replaced.","Cargo Mach.","MARPOL Related","Equipment Related","6.13","Low","","","ink ribbon renewed.","2019-05-10","","Completed","2019-05-09","No","No","No","Internal"]
[null,null,null,null,5024,"49_25/10/2019 5:45:12 PM","2019-05-07","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","pilot ladder should be in compliance with IMO resolution A.1045(27),please confirm the same.Attached message for reference.","Miscellaneous","General Appearance","Equipment Related","5.47","Medium","","","Vessel pilot ladder complying with IMO requirement.","2019-05-30","","Completed","2019-05-10","No","No","No","Internal"]
[null,null,null,null,5057,"49_26/10/2019 7:22:19 AM","2019-05-07","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","STBD side conduit pipe near LB, electrical wire pocket needs to be filled with electrical putty.","Miscellaneous","General Appearance","Equipment Related","11.1","High","","","Done","2019-05-30","","Completed","2019-05-25","No","No","No","Internal"]
[null,null,null,null,5071,"49_27/10/2019 2:51:21 AM","2019-05-07","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Port side bunker high level alarm electrical pipe support bar wasted, needs renewal.","Miscellaneous","General Appearance","External Factors","11.1","High","","","renewed","2019-08-08","","Completed","2019-06-15","No","No","No","Internal"]
[null,null,null,null,5073,"49_27/10/2019 3:23:25 AM","2019-05-07","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Electrical wire support bar for emg lighting near LB launching proceduers wasted, needs renewal.","Miscellaneous","General Appearance","External Factors","11.1","High","","","Renewed","2019-08-08","","Completed","2019-06-15","No","No","No","Internal"]
[null,null,null,null,5134,"49_27/10/2019 3:24:28 PM","2019-05-08","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","WS lathe machine should fabricate transparent safety shield to avoid injury to eye of personnel carrying out the job.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.12","Very High","","","No transparent safety shield available on board, item will be added to ER store requisition.","2019-06-05","RESP190064","Completed","2019-08-29","No","No","No","Internal"]
[null,null,null,null,4938,"49_25/10/2019 7:19:54 PM","2019-05-08","Defect","Ship Staff","Ship Staff Insp.","BRIDGE WING DECK PAINT COATING CRACKED AND FLAKING OUT.","Hull & Tanks","General Appearance","External Factors","11.1","High","","","DECK TO BE CHIPPED AND HYDROBLASTED ,BUFFED ,TWO COATS OF PRIMER AND FINAL COAT TO BE APPLIED.","2019-05-30","","Completed","2019-05-29","No","No","No","Internal"]
[null,null,null,null,4951,"49_26/10/2019 5:13:55 AM","2019-05-08","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Notice near 15ppm should mention \"not to be operated without permission of Master and CE.","E/R - Aux. Engine","Eng. / Strg. Comp.","Inappropriate Procedure","6.3","Low","","","New poster placed near OWS","2019-05-08","","Completed","2019-05-08","No","No","No","Internal"]
[null,null,null,null,4952,"49_26/10/2019 5:16:10 AM","2019-05-08","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Fire Bilge & ballast pump priming arrangement missing","E/R - Aux. Engine","Eng. / Strg. Comp.","Inappropriate Procedure","2.7","High","","","vacuum pump overhauled. Its in operation","2019-05-08","","Completed","2019-05-08","No","No","No","Internal"]
[null,null,null,null,4953,"49_26/10/2019 5:18:02 AM","2019-05-08","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Spring for DB tank sounding cap missing","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.34","High","","","New spring put in place","2019-05-15","","Completed","2019-05-10","No","No","No","Internal"]
[null,null,null,null,4954,"49_26/10/2019 5:19:26 AM","2019-05-08","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Permanent RA for carrying out fuel v/v pressure test to be pasted neat the testing m/c recommended.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.25","Very High","","","RA made and posted near testing m/c","2019-05-08","","Completed","2019-05-08","No","No","No","Internal"]
[null,null,null,null,4955,"49_26/10/2019 5:35:27 AM","2019-05-08","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ODME printer cartridge needs to be replaced.","Elect. Mach. & Equip.","Cargo / Ballast Systems","Equipment Related","6.3","Low","","","ODME printer cartridge renewed.","2019-05-20","","Completed","2019-05-09","No","No","No","Internal"]
[null,null,null,null,4956,"49_26/10/2019 5:38:22 AM","2019-05-08","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Fwd air cooler SW inlet pipe leaking","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.2","Low","","","Fwd air cooler SW inlet pipe leak rectified","2019-05-25","","Completed","2019-05-12","No","No","No","Internal"]
[null,null,null,null,5018,"49_25/10/2019 8:25:11 AM","2019-05-08","Defect","Ship Staff","Ship Staff Insp.","RESCUE STRETCHER IN PUMP ROOM STRAP BROKEN.","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.3","Low","","","SPARE STRETCHER RENEWED, BROKEN STRECHER REMOVED.","2019-05-10","","Completed","2019-05-08","No","No","No","Internal"]
[null,null,null,null,5019,"49_25/10/2019 8:30:03 AM","2019-05-08","Defect","Ship Staff","Ship Staff Insp.","RUBBER PACKING FOR WEATHERTIGHT DOORS OF CO2 ROOM AND FORECASTLE STORE FOUND CRACKED AND BROKEN.","Hull & Tanks","General Appearance","Equipment Related","11.3","Medium","","","RUBBER PACKING RENEWED.","2019-05-10","","Completed","2019-05-10","No","No","No","Internal"]
[null,null,null,null,5020,"49_25/10/2019 8:36:06 AM","2019-05-08","Defect","Ship Staff","Ship Staff Insp.","CHINA PASSAGE STOWED WITH GREASED BUCKETS, OLD PAINT DRUMS, WOODEN PALLETS, ROPES DIRECTLY BELLOW FUNNEL.","Miscellaneous","General Appearance","Human Error","11.5","Medium","","","OLD BUCKETS AND DRUMS CLEANED AND STORED IN LOCKER, WOODEN PALLETS AND ROPES STORED IN STEERING FLAT, CHINA PASSAGE CLEARED OF DEBRIS.","2019-05-11","","Completed","2019-05-11","No","No","No","Internal"]
[null,null,null,null,5025,"49_25/10/2019 5:50:12 PM","2019-05-08","Defect","Ship Staff","Ship Staff Insp.","RUBBER PACKING FOR MUSHROOM VENTS FOUND BROKEN FOR SANITARY EXHAUST VENT ,STEERING FLAT VENTS.","LSA / FFA","Safety / LSA / FFA","Equipment Related","11.3","Medium","","","RUBBER PACKING RENEWED FOR COMPLETD SEALING ON CLOSURE.","2019-05-12","","Completed","2019-05-12","No","No","No","Internal"]
[null,null,null,null,5037,"49_26/10/2019 5:40:12 AM","2019-05-08","Defect","Ship Staff","Ship Staff Insp.","pneumatic driven pump for AE not operational","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.12","Very High","","","Pump and air motor overhauled","2019-05-25","","Completed","2019-05-17","No","No","No","Internal"]
[null,null,null,null,5074,"49_27/10/2019 3:25:51 AM","2019-05-08","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","STBD side conduit pipe nar LB, electrical wire pocket needs to be filled with electrical putty.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.23","Medium","","","Renewed","2019-08-08","","Completed","2019-06-15","No","No","No","Internal"]
[null,null,null,null,5029,"49_25/10/2019 6:16:06 PM","2019-05-09","Defect","Ship Staff","Ship Staff Insp.","PV Breaker to be de-rusted and painted, Check for calibration.","Inert Gas","Cargo / Ballast Systems","Equipment Related","8.32","Low","","","PV Breaker de-rusted, inspected, liquid checked, full final coat painted, stencilled.","2019-06-30","","Completed","2019-05-17","No","No","No","Internal"]
[null,null,null,null,5032,"49_25/10/2019 6:25:43 PM","2019-05-09","Defect","Ship Staff","Ship Staff Insp.","2C, 5C COT and 2s COT PV valve pressure side leaking.","Inert Gas","Cargo / Ballast Systems","Equipment Related","8.32","Low","","","PV valves for 2C, 5C and 2S COT lapped and rectified, spare PV valve lapped and kept ready for emergency.","2019-05-30","","Completed","2019-05-21","No","No","No","Internal"]
[null,null,null,null,5036,"49_25/10/2019 7:15:31 PM","2019-05-09","Defect","Ship Staff","Ship Staff Insp.","ALL COT PV VALVES NEED DERUSTING AND PAINTING.","Inert Gas","Cargo / Ballast Systems","Equipment Related","8.32","Low","","","PV VALVES PIPES AND STAND DERUSTING AND PAINTING IN PROGRESS.","2019-06-30","","Completed","2019-05-30","No","No","No","Internal"]
[null,null,null,null,5038,"49_26/10/2019 5:45:43 AM","2019-05-09","Defect","Ship Staff","Ship Staff Insp.","Emergency generator exhaust pipe badly corroded.","LSA / FFA","General Appearance","Equipment Related","11.6","Medium","","","Vent pipe renewed.","2019-06-15","","Completed","2019-05-14","No","No","No","Internal"]
[null,null,null,null,5039,"49_26/10/2019 5:42:12 AM","2019-05-09","Defect","Ship Staff","Ship Staff Insp.","Main cooling SW pump no.2 mech seal leaking","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","main SW cooling pipe cleaned, no leak from seal","2019-06-15","","Completed","2019-05-27","No","No","No","Internal"]
[null,null,null,null,5040,"49_26/10/2019 5:51:45 AM","2019-05-09","Defect","Ship Staff","Ship Staff Insp.","Laggine at many places to be ratched up properly","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.25","Very High","","","Lagging renewed.","2019-06-15","","Completed","2019-05-27","No","No","No","Internal"]
[null,null,null,null,5041,"49_26/10/2019 5:49:26 AM","2019-05-09","Defect","Ship Staff","Ship Staff Insp.","EGB feed pump no.2 bearings need to be replaced.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.25","Very High","","","Bearing renewed","2019-06-15","","Completed","2019-05-21","No","No","No","Internal"]
[null,null,null,null,5046,"49_26/10/2019 6:04:50 AM","2019-05-09","Defect","Ship Staff","Ship Staff Insp.","Main engine unit #5 indicator valve leak","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.25","Very High","","","Main engine unit #5 indicator valve renewed","2019-06-15","","Completed","2019-05-30","No","No","No","Internal"]
[null,null,null,null,5066,"49_27/10/2019 2:14:20 AM","2019-05-09","Defect","Ship Staff","Ship Staff Insp.","Mast Riser derusting and paintaing to be done.","Inert Gas","Cargo / Ballast Systems","Equipment Related","8.19","High","","","Mast Riser derusted and painted full coat.","2019-08-09","","Completed","2019-06-10","No","No","No","Internal"]
[null,null,null,null,5067,"49_27/10/2019 2:25:51 AM","2019-05-09","Defect","Ship Staff","Ship Staff Insp.","Old man roller for SBM chain forecastle frozen, need to be freed.","Miscellaneous","Mooring","Equipment Related","","","","","Freed, greased Dismantled.","2019-08-09","","Completed","2019-06-14","No","No","No","Internal"]
[null,null,null,null,5079,"49_27/10/2019 3:57:38 AM","2019-05-09","Defect","Ship Staff","Ship Staff Insp.","Main SW upmp no.1 motor bearings to renewed as its making noise","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.24","Low","","","Bearing renewed","2019-08-08","","Completed","2019-06-19","No","No","No","Internal"]
[null,null,null,null,5080,"49_27/10/2019 4:00:33 AM","2019-05-09","Defect","Ship Staff","Ship Staff Insp.","FWG/ Deck seal pump cover broken","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.22","Low","","","Await spares/ Broken cover fabricated","2019-08-08","RESP195061","Completed","2019-06-16","No","No","No","Internal"]
[null,null,null,null,5083,"49_27/10/2019 4:05:35 AM","2019-05-09","Defect","Ship Staff","Ship Staff Insp.","AE #1 Starting air pressure regulating valve found faulty","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.12","Very High","","","Same renewed with overhauled spare","2019-06-16","","Completed","2019-06-15","No","No","No","Internal"]
[null,null,null,null,5095,"49_27/10/2019 5:33:12 AM","2019-05-09","Defect","Ship Staff","Ship Staff Insp.","Fridge compressor sump oil for both compressor needs to be changed","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.14","Medium","","","oil renewed","2019-08-08","","Completed","2019-07-01","No","No","No","Internal"]
[null,null,null,null,5101,"49_27/10/2019 6:37:50 AM","2019-05-09","Defect","Ship Staff","Ship Staff Insp.","Aux boiler DP transmitter valves not holding","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.21","Medium","","","valves renewed","2019-08-08","","Completed","2019-07-16","No","No","No","Internal"]
[null,null,null,null,5108,"49_27/10/2019 12:46:53 PM","2019-05-09","Defect","Ship Staff","Ship Staff Insp.","AC compressor sump oil needs to be replaced","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.13","Very High","","","Oil renewed","2019-08-08","","Completed","2019-07-22","No","No","No","Internal"]
[null,null,null,null,5076,"49_27/10/2019 3:30:40 AM","2019-05-10","Defect","Ship Staff","Ship Staff Insp.","Boiler water circulating pump discharge valve to no.1 BLR not holding","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.22","Low","","","Same valve renewed with new spare valves","2019-06-30","","Completed","2019-06-24","No","No","No","Internal"]
[null,null,null,null,5068,"49_27/10/2019 2:34:13 AM","2019-05-12","Defect","Ship Staff","Ship Staff Insp.","Bridge doors not gas tight.","Miscellaneous","General Appearance","External Factors","11.6","Medium","","","Rollers adjusted for proper sealing against rubber packing.","2019-08-12","","Completed","2019-06-06","No","No","No","Internal"]
[null,null,null,null,5028,"49_25/10/2019 6:07:23 PM","2019-05-13","Defect","Ship Staff","Ship Staff Insp.","AIR REGULATOR TO BE FIXED FOR CARGO SEACHEST EXXON TEST, PICTORIAL TEST, PROCEDURE TO BE PASTED NEAR CARGO SEACHEST VALVE.","Miscellaneous","Cargo / Ballast Systems","Equipment Related","8.25","Very High","","","AIR REGULATOR FIXED AND TEST PROCEDURES PASTED.","2019-05-30","","Completed","2019-05-15","No","No","No","Internal"]
[null,null,null,null,5104,"49_27/10/2019 6:55:29 AM","2019-05-15","Defect","Ship Staff","Ship Staff Insp.","SUPPORT PIPE FOR MOORING WINCH OPERATOR STANDING PLATFORM HOLED AND WASTED FOR STERN MOORING WINCH NO 7","Deck - Mooring Machinery","Mooring","Equipment Related","9.15","Medium","","","COLD WORK REPAIR CARRIED OUT. STRENGTHEN THE SUPPORT PIPE AND PAINTING.","2019-08-15","","Completed","2019-07-29","No","No","No","Internal"]
[null,null,null,null,5035,"49_25/10/2019 7:08:20 PM","2019-05-16","Defect","Ship Staff","Ship Staff Insp.","AIR HOSE FOR PORT SIDE PILOT LADDER SHIFTING REEL CRACKED AND BROKEN.","Miscellaneous","Safety / LSA / FFA","Equipment Related","5.27","Medium","","","AIR HOSE REPLASED.","2019-05-30","","Completed","2019-05-24","No","No","No","Internal"]
[null,null,null,null,5072,"49_27/10/2019 2:39:05 AM","2019-05-20","Defect","Ship Staff","Ship Staff Insp.","Scupper pipes on deck to be derusted and painted, Scupper plugs maintenance, Greasing and numbering to be carried.","Hull & Tanks","General Appearance","Equipment Related","","","","","Scupper plugs and Scupper pipes derusted and maintenance carried out.","2019-08-20","","Completed","2019-06-15","No","No","No","Internal"]
[null,null,null,null,4935,"49_24/10/2019 7:15:36 PM","2019-05-21","Defect","Ship Staff","Ship Staff Insp.","Unit no. 7 top piston ring broken at butt.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.12","Very High","","","Piston renewed with overhauled, ring renewed.","2019-11-15","","Completed","2019-11-11","No","No","No","Internal","Pls continue with monitoring of the scavenge temperature and keep this office updated should there be any change to same. "]
[null,null,null,null,5042,"49_26/10/2019 5:53:28 AM","2019-05-21","Defect","Ship Staff","Ship Staff Insp.","Drinking water pump leaking","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.47","Medium","","","Pump overhauled","2019-05-25","","Completed","2019-05-23","No","No","No","Internal"]
[null,null,null,null,5043,"49_26/10/2019 5:55:14 AM","2019-05-29","Defect","Ship Staff","Ship Staff Insp.","No2 waste oil tank sounding float not working","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.47","Medium","","","Float wire renewed","2019-06-15","","Completed","2019-05-29","No","No","No","Internal"]
[null,null,null,null,5077,"49_27/10/2019 3:33:52 AM","2019-06-15","Defect","Ship Staff","Ship Staff Insp.","Galley A/C blower casing damaged.","E/R - Aux. Mach.","General Appearance","Equipment Related","10.47","Medium","","","Rectified","2019-08-08","","Completed","2019-06-24","No","No","No","Internal"]
[null,null,null,null,5078,"49_27/10/2019 3:55:37 AM","2019-06-16","Defect","Ship Staff","Ship Staff Insp.","Main SW pump no.1 mechanical seal leaky","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.47","Medium","","","Mechanical seal renewed","2019-08-08","","Completed","2019-06-19","No","No","No","Internal"]
[null,null,null,null,5081,"49_27/10/2019 4:02:35 AM","2019-06-16","Defect","Ship Staff","Ship Staff Insp.","ME turbocharger grit washing pipe found choked","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.47","Medium","","","Same rectified","2019-06-30","","Completed","2019-06-21","No","No","No","Internal"]
[null,null,null,null,5082,"49_27/10/2019 4:04:19 AM","2019-06-17","Defect","Ship Staff","Ship Staff Insp.","AE No.2 unit #2 exhaust temperature high","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.47","Medium","","","unit #2 FO pump renewed","2019-06-30","","Completed","2019-06-19","No","No","No","Internal"]
[null,null,null,null,5087,"49_27/10/2019 4:29:12 AM","2019-06-25","Defect","Ship Staff","Ship Staff Insp.","Steam leak near incinerator","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.47","Medium","","","rectified","2019-06-30","","Completed","2019-06-26","No","No","No","Internal"]
[null,null,null,null,5086,"49_27/10/2019 4:17:06 AM","2019-06-26","Defect","Ship Staff","Ship Staff Insp.","Steam leak near FWG","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.47","Medium","","","rectified","2019-06-30","","Completed","2019-06-26","No","No","No","Internal"]
[null,null,null,null,5123,"49_27/10/2019 1:39:36 PM","2019-06-27","Defect","Ship Staff","Ship Staff Insp.","STBD windlass pinion and gear slipping at particular instances.","Deck - Mooring Machinery","Mooring","Equipment Related","9.24","Medium","","","To check the backlash of gear checked and both pinion bearings renewed.","2019-07-30","","Completed","2019-08-12","No","No","No","Internal"]
[null,null,null,null,5096,"49_27/10/2019 5:34:30 AM","2019-07-01","Defect","Ship Staff","Ship Staff Insp.","Oil leaking from AE F.O. duplex filter changing lever","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.47","Medium","","","O ring renewed","2019-07-03","","Completed","2019-07-02","No","No","No","Internal"]
[null,null,null,null,5097,"49_27/10/2019 5:36:19 AM","2019-07-03","Defect","Ship Staff","Ship Staff Insp.","AE1 FO inlet valve bonnet leaky","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.47","Medium","","","Bonnet gasket renewed","2019-07-03","","Completed","2019-07-03","No","No","No","Internal"]
[null,null,null,null,5098,"49_27/10/2019 6:29:27 AM","2019-07-03","Defect","Ship Staff","Ship Staff Insp.","Incinerator service tank's drain choked","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.47","Medium","","","Tank to be cleaned","2019-07-15","","Completed","2019-07-06","No","No","No","Internal"]
[null,null,null,null,5100,"49_27/10/2019 6:33:06 AM","2019-07-03","Defect","Ship Staff","Ship Staff Insp.","Upper deck and mess room's drinking water fountain not working. Filter to be cleaned","E/R - Aux. Mach.","MLC Related","Equipment Related","10.47","Medium","","","Fountain working and filter cleaned","2019-07-10","","Completed","2019-07-05","No","No","No","Internal"]
[null,null,null,null,5109,"49_27/10/2019 12:52:41 PM","2019-07-03","Defect","Ship Staff","Ship Staff Insp.","PORT windlass FWD motor has excessive hydaulic oil leak.","Deck - Mooring Machinery","Mooring","Equipment Related","9.21","Medium","","","Forward motor complet overhauling carried out.","2019-08-15","","Completed","2019-07-22","No","No","No","Internal"]
[null,null,null,null,5124,"49_27/10/2019 1:44:00 PM","2019-07-05","Defect","Ship Staff","Ship Staff Insp.","STBD windlass aft motor end cover wasted.","Deck - Mooring Machinery","Mooring","Equipment Related","9.25","Low","","","Reqn, Raised for new cover.Temparory repairs carried out and motor tried out found no leak.","2019-08-30","RESP190056","Completed","2019-08-12","No","No","No","Internal"]
[null,null,null,null,5099,"49_27/10/2019 6:30:57 AM","2019-07-05","Defect","Ship Staff","Ship Staff Insp.","ME LO purifier inlet temperature not rising","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.47","Medium","","","To be cleaned","2019-07-06","","Completed","2019-07-06","No","No","No","Internal"]
[null,null,null,null,5120,"49_27/10/2019 1:28:03 PM","2019-07-13","Defect","Ship Staff","Ship Staff Insp.","Garbage bins at garbage point not seal tight.","Miscellaneous","General Appearance","Equipment Related","11.2","Medium","","","Hing and securing arrangement prepared.","2019-08-15","","Completed","2019-08-10","No","No","No","Internal"]
[null,null,null,null,5105,"49_27/10/2019 6:58:51 AM","2019-07-13","Defect","Ship Staff","Ship Staff Insp.","DECK SEAL FLANGE FOR HIGH LEVEL SENSOR HOUSING HOLED.","Inert Gas","Cargo / Ballast Systems","Equipment Related","8.12","Medium","","","NEW FLANGE FABRICATED.","2019-08-15","","Completed","2019-07-18","No","No","No","Internal"]
[null,null,null,null,5106,"49_27/10/2019 7:08:14 AM","2019-07-13","Defect","Ship Staff","Ship Staff Insp.","GANGWAY PORT SIDE LEVER BODY FOR SWING IN/OUT BROKEN.","Deck - Machinery","General Appearance","Equipment Related","11.4","Very High","","","SPARE LEVER BODY REPLACED AND TRIED OUT.","2019-08-15","","Completed","2019-07-25","No","No","No","Internal"]
[null,null,null,null,5107,"49_27/10/2019 7:11:55 AM","2019-07-13","Defect","Ship Staff","Ship Staff Insp.","CARGO MANIFOLD PORT AND STBD GAUGE COCKS WHEELS BROKEN.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.32","Low","","","WHEELS FABRICATED AND INSTALLED.","2019-07-15","","Completed","2019-07-28","No","No","No","Internal"]
[null,null,null,null,5110,"49_27/10/2019 12:54:07 PM","2019-07-19","Defect","Ship Staff","Ship Staff Insp.","No1 boiler starboard gauge glass leaky","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.47","Medium","","","Gauge glass renewed","2019-08-30","","Completed","2019-07-20","No","No","No","Internal"]
[null,null,null,null,5121,"49_27/10/2019 1:32:57 PM","2019-08-06","Defect","Ship Staff","Ship Staff Insp.","Mooring winch MW5 inlet line holded.","Deck - Mooring Machinery","Mooring","Equipment Related","9.12","Medium","","","Inlet pipeline to dimantel and welded and fixed back in position.","2019-08-15","","Completed","2019-08-10","No","No","No","Internal"]
[null,null,null,null,5122,"49_27/10/2019 1:35:36 PM","2019-08-06","Defect","Ship Staff","Ship Staff Insp.","Mooring winch MW6 inlet line valve leaking.","Deck - Mooring Machinery","Mooring","Equipment Related","9.21","Medium","","","Inlet valve to repair and fixed back.","2019-08-15","","Completed","2019-08-10","No","No","No","Internal"]
[null,null,null,null,5114,"49_27/10/2019 1:03:10 PM","2019-08-06","Defect","Ship Staff","Ship Staff Insp.","MSB room AC sea water inlet pipe holed","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.31","Very High","","","pipe section to be renewed","2019-08-15","","Completed","2019-08-07","No","No","No","Internal"]
[null,null,null,null,5115,"49_27/10/2019 1:04:41 PM","2019-08-06","Defect","Ship Staff","Ship Staff Insp.","ECR AC sea water inlet pipe holed","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.21","Medium","","","Pipe section to be renewed","2019-08-15","","Completed","2019-08-07","No","No","No","Internal"]
[null,null,null,null,5116,"49_27/10/2019 1:09:30 PM","2019-08-06","Defect","Ship Staff","Ship Staff Insp.","Control air has too much water content","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.47","Medium","","","Control air drier filter to be cleaned","2019-08-15","","Completed","2019-08-06","No","No","No","Internal"]
[null,null,null,null,5117,"49_27/10/2019 1:12:27 PM","2019-08-06","Defect","Ship Staff","Ship Staff Insp.","Water leaking from hydroblaster shaft","Miscellaneous","General Appearance","Equipment Related","11.5","Medium","","","Oring to be renewed.","2019-08-15","","Completed","2019-08-06","No","No","No","Internal"]
[null,null,null,null,8462,"49_20/12/2019 1:03:50 AM","2019-08-19","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","VDR Microphone & BNWAS reset button not available on bridge wings","Navigation - VDR / BNWAS","Navigation","Equipment Related","4.7","High","","","Job Has been added in REFMAN for next scheduled Dry Dock.","2020-12-31","","Completed","2020-11-24","Yes","No","No","Internal","Noted.  Tech. Supt  please check if job has indeed been updated in REFMAN."]
[null,null,null,null,8475,"49_20/12/2019 8:23:52 AM","2019-08-20","Defect","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","1 SCBA bottle unit for Helicopter equipment stowed inside midship locker store was noted with defective demand valve whilst testing.","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.43","High","","","New demand valve received in Singapore and fitted.","2019-08-31","","Completed","2019-08-23","No","No","No","External"]
[null,null,null,null,8464,"49_20/12/2019 1:17:15 AM","2019-08-21","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Missing / Poor condition of anti-skid paint coating at mooring area.","Deck - Mooring Machinery","Mooring","Inappropriate Procedure","11.3","Medium","","","Vessel received Anti-skid paint on 05-Dec-19 and has already completed de-rusting & primering of mooring area. Final coating with antiskid paint completed.","2020-01-31","","Completed","2020-11-16","No","No","No","External","Please revert with updated status for said job. It has already been more than 15 months since the defect was recorded but to date still not completed.  We suggest that you provide a realistic target date."]
[null,null,null,null,8477,"49_20/12/2019 8:35:48 AM","2019-08-21","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Entries in the cargo log not in line with the recommended entries mention at the start of the book. No record of cross-checks made by OOW for the line ups.","Cargo Mach.","Cert. & Docu.","Human Error","8.5","Very High","","","Standard guidelines provided by company regarding entry in log books has been discussed and followed. During Pre-Arrival cargo meeting same to be discussed always.","2019-09-30","","Completed","2019-09-13","No","No","No","Internal"]
[null,null,null,null,8478,"49_20/12/2019 11:09:43 AM","2019-08-21","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","MBL markings not present on the mooring winches (Refer Mooring equipment guidelines 4)","Deck - Mooring Machinery","Mooring","Knowledge Based","9.7","Medium","","","MEG Ed.4 has been referred and the required markings carried out. ","2019-09-30","","Completed","2019-09-14","No","No","No","Internal"]
[null,null,null,null,9991,"49_21/01/2020 5:17:22 AM","2019-08-23","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Leak on port windlass under shaft sea.","Deck - Mooring Machinery","Mooring","Equipment Related","9.14","Medium","","","Leak Rectified.","2019-09-10","","Completed","2019-09-05","No","No","No","Internal"]
[null,null,null,null,9992,"49_21/01/2020 5:27:46 AM","2019-08-23","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Bunker line near the pump room is heavily rusted from bottom. Proper hydro test of Bunker line to be carried out. Area to be wire brushed and painted. ","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.4","Very High","","","Buffing and painting carried out.","2019-09-30","","Completed","2019-09-10","No","No","No","Internal"]
[null,null,null,null,9993,"49_21/01/2020 5:45:40 AM","2019-08-23","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","The Deck and engine stores on the vessel are disorganised with lot of scrap material lying in the stores.  The old spares/ stores are to be segregated and proper inventories are to be taken and updated in the PMS. ","Miscellaneous","General Appearance","Inappropriate Procedure","11.8","Low","","","Stores arranged & inventories have been taken and updated.","2019-09-30","","Completed","2019-09-15","No","No","No","Internal"]
[null,null,null,null,9994,"49_21/01/2020 5:53:54 AM","2019-08-23","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Cargo Area is dirty, to be cleaned.","Miscellaneous","General Appearance","Inappropriate Procedure","11.3","Medium","","","Cleaned the area.","2019-09-30","","Completed","2019-08-24","No","No","No","Internal"]
[null,null,null,null,9995,"49_20-Jan-20 7:07:24 AM","2019-08-23","Observation","Owner / Marine / Tech. Suptd.","Ship Staff Insp.","MONO RAILING HOISTING MOTOR MALFUNCTING ","Deck - Machinery","Eng. / Strg. Comp.","Human Error","10.3","Medium","","","SAME RECTIFIED","2019-08-25","","Completed","2019-08-24","No","No","No","Internal"]
[null,null,null,null,9997,"49_21/01/2020 5:11:07 AM","2019-08-23","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","MW7 on Poop Deck is leaking from the flange. To be rectified.      Cover of gears for all winches and windlass are in poor condition.","Deck - Mooring Machinery","Mooring","Equipment Related","9.14","Medium","","","leak rectified. Cover gears of all winches in aft repaired.","2020-01-30","","Completed","2020-01-15","No","No","No","Internal"]
[null,null,null,null,5135,"49_27/10/2019 3:27:04 PM","2019-08-23","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","MW7 in poop deck is leaking from flange.","Deck - Mooring Machinery","Mooring","Equipment Related","9.14","Medium","","","Hydraulic leak rectified.","2019-09-22","","Completed","2019-09-03","No","No","No","Internal"]
[null,null,null,null,5137,"49_27/10/2019 3:32:39 PM","2019-08-23","Defect","Ship Staff","Ship Staff Insp.","Unit 7 and 5 were found dry during the scavenge inspection. The CLO lubrication to be increased for these units and closely monitored","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","8.14","Very High","","","CLO setting increased","2019-08-30","","Completed","2019-08-26","No","No","No","Internal"]
[null,null,null,null,5139,"49_27/10/2019 3:39:48 PM","2019-08-23","Defect","Ship Staff","Ship Staff Insp.","Arrangement for waer washing of AE turbocharger does not have a drain arrangement","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","8.47","Very High","","","As per manual no drain but water flow regulating valve to maintain the flow. Cycle carried out 3 times based on........","2019-10-22","","Completed","2019-08-23","No","No","No","Internal"]
[null,null,null,null,5141,"49_27/10/2019 3:44:33 PM","2019-08-23","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Noon log alarm printer in ECR not working","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","8.21","High","","","noon log printer working satisfactorily","2019-10-22","","Completed","2019-09-13","No","No","No","Internal"]
[null,null,null,null,5143,"49_27/10/2019 3:50:19 PM","2019-08-23","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Covers for the hydraulic boxes on deck have not been blasted and painted from the bottom at the.........","Deck - Machinery","General Appearance","Equipment Related","","","","","Same to carried out.Silica get to be placed inside the boxes.","2019-11-22","","Completed","2019-09-20","No","No","No","Internal","Noted"]
[null,null,null,null,5153,"49_27/10/2019 4:36:18 PM","2019-08-23","Defect","Ship Staff","Ship Staff Insp.","Auxboiler no2 steam stop valve gland is leaking. To be rectified.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Bonnet gasket renewed. Leak rectified.","2019-10-22","","Completed","2019-10-16","No","No","No","Internal"]
[null,null,null,null,4928,"49_24/10/2019 6:29:35 PM","2019-08-23","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","The covers for the hydraulic boxes have damaged lips.","Deck - Machinery","Cargo / Ballast Systems","External Factors","11.1","High","","","All hydraulic box covers taken to ER workshop and repairs carried out. All covers derusted and painted 2 primer and topcoat.","2020-03-31","","Completed","2020-04-25","No","No","No","Internal",""]
[null,null,null,null,4930,"49_24/10/2019 6:47:57 PM","2019-08-23","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Paint is peeling of at several locations on main deck.","Deck - Machinery","General Appearance","External Factors","11.1","High","","","same been blasted/ buffed as found necessary and repainted.","2020-02-28","","Completed","2019-12-18","No","No","No","Internal","Pls revert with update on progress of the works, to date, based on percentage of job completed.                                                                                                                                                                                                                                                                                                                                                                                                                           "]
[null,null,null,null,4931,"49_24/10/2019 6:52:14 PM","2019-08-23","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","All rusted areas on main deck and poop deck to be spot blasted and painted with two coats of primer and one final coat of top.","Deck - Machinery","General Appearance","External Factors","11.1","High","","","All rusted areas on poop deck been spot blasted and painted with two coats of primer and one final coat of top.","2020-02-28","","Completed","2020-11-19","No","No","No","Internal","Noted and Target date revised."]
[null,null,null,null,4932,"49_24/10/2019 6:56:25 PM","2019-08-23","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Pipe line supports and U clamps on deck are rusted.","Deck - Pipe / Fittings","General Appearance","External Factors","11.5","Medium","","","The pipeline & associated supports including U clamp renewal completed and few postponed to Drydock.","2020-04-22","","Completed","2020-11-18","No","No","No","Internal","Please revert with updated status for said defect and provide a realistic target date.  It has been approx. 15 months since the job was created."]
[null,null,null,null,5142,"49_27/10/2019 3:46:20 PM","2019-08-26","Defect","Ship Staff","Ship Staff Insp.","ECR noon log printer not working","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","cartridge renewed","2019-11-20","","Completed","2019-09-12","No","No","No","Internal"]
[null,null,null,null,5144,"49_27/10/2019 4:14:53 PM","2019-08-26","Defect","Ship Staff","Ship Staff Insp.","No.1 ballast pump mechanical seal leak. ","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.11","Medium","","","Seal renewed.","2019-09-30","","Completed","2019-09-23","No","No","No","Internal"]
[null,null,null,null,4927,"49_24/10/2019 6:24:13 PM","2019-08-26","Defect","Ship Staff","Ship Staff Insp.","Fire bilge and ballast pump suction valve not holding.","Miscellaneous","Cargo / Ballast Systems","Equipment Related","10.31","Very High","","","Suction valve insepcted and found ok. Discharge valve to overbaod/aft peak is not holding. ","2020-02-15","RESP20037","Completed","2020-04-29","Yes","No","No","Internal","Same to be included in dry-docking specification c/w details of the valve."]
[null,null,null,null,5136,"49_27/10/2019 3:30:31 PM","2019-08-27","Defect","Ship Staff","Ship Staff Insp.","Observed two holes in STBD side pilot ladder pneumatic line.","Deck - Machinery","General Appearance","Equipment Related","9.15","Medium","","","Section disconnected, repaired and fitted back.","2019-09-10","","Completed","2019-09-05","No","No","No","Internal"]
[null,null,null,null,8467,"49_Mon Oct 28 2019 06:34:23 GMT+0000 (Coordinated Universal Time)","2019-08-27","Defect","Ship Staff","Ship Staff Insp.","Unit no 2 top piston ring broken at butt","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.12","Very High","","","piston renewed with overhauled spare piston and piston rings are renewed","2019-11-30","","Completed","2019-11-07","No","No","No","Internal"]
[null,null,null,null,4937,"49_2019-10-28 06:34:23.000","2019-08-27","Defect","Ship Staff","Ship Staff Insp.","Unit no 2 top piston ring broken at butt","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.12","Very High","","","UNIT DECARB CARRIED OUT","2019-11-30","","Completed","2019-11-09","No","No","No","Internal","Pls continue to monitor the scavenge temperature and update this office accordingly."]
[null,null,null,null,8465,"49_20/12/2019 12:01:06 PM","2019-08-28","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","3 of the 5 nos of SCBA face masks noted slightly opaque","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.43","High","","","SCBA masks recieved and same replaced.","2020-01-30","","Completed","2020-02-06","No","No","No","Internal","Noted. Will expedite."]
[null,null,null,null,8479,"49_20/12/2019 11:48:09 AM","2019-08-28","Defect","Owner / Marine / Tech. Suptd.","Nav Audit / Verification","Only the internal history of the FE800 Furuno Echosounder is available, No external recording facility available","Navigation - Echo Sounder / Speed Log","Navigation","Equipment Related","4.19","Low","","","The vessel has a Data recroding software (FE800 DATA RECORDING SYSTEM) which is malfunctioning after the upgradation of the Personal computer to Windows 7 OS. Vessel is working on resolving the isue so as to enable data saving facility for future referance. Vessel has raised a servie requisition for IT support to rectify the issue. \n\nHowever, for the time being the echo sounder data is being recorded by the Master ECDIS which can save the data for 90 days and the vessel is writing down the depths at critical stages in the Bridge bell book.","2019-09-15","","Completed","2019-09-12","No","No","No","Internal"]
[null,null,null,null,8480,"49_20/12/2019 11:50:31 AM","2019-08-28","Defect","Owner / Marine / Tech. Suptd.","Nav Audit / Verification","Pre Departure tests and checks for GMDSS equipment not carried out. \n\nDeparture steering gear tests: 3 monthly steering gear (due on 23rd Aug 2019) not carried out","Navigation - GMDSS & Communication","Navigation","Human Error","4.23","High","","","-Steering gear test carried out on first available oppurtunity as per regulations. \n\nFound in good working order. \n\nNecessary entries made and the test was documented. \n\n-GMDSS departure tests carried out as well by the GMDSS officer. GMDSS Officer instructed to not let such a lapse occur again and to ensure that the pre departure tests are carried out diligently.","2019-09-15","","Completed","2019-09-12","No","No","No","Internal"]
[null,null,null,null,8481,"49_20/12/2019 11:54:08 AM","2019-08-28","Defect","Owner / Marine / Tech. Suptd.","Nav Audit / Verification","Celestial observations were not practiced by each member of the bridge team ","Navigation - Others","Navigation","Human Error","4.2","Medium","","","Celestial observations practised by all OOW and logged down. \n\nComparison has been carried out with the position obtained by the Celestial observation and the GPS position at that instant. Error deemed to be slight and acceptable. ","2019-09-15","","Completed","2019-09-12","No","No","No","Internal"]
[null,null,null,null,8466,"49_20/12/2019 12:07:54 PM","2019-08-29","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Fire Doors for the emergency exit in the E/R at the steering gear and at the bottom platform need renewal of fittings and door closers. (Doors not closing fully)\n\n5 nos of door around accommodation with door closers need renewal of door closers, 8 nos need adjustments .  Galley doors to the mess-rooms donot have door closers.","Accommodation","Structural Condn. / WT integrity ","Equipment Related","11.14","Medium","","","Door handle removed , overhauled and fitted back, one renewed.Door closer adjusted  ","2020-02-13","RESP190113","Completed","2020-02-13","No","No","No","Internal","Noted. We will supply the door closers during the vessel's Next Storing at Singapore."]
[null,null,null,null,8482,"49_20/12/2019 11:56:25 AM","2019-08-29","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","LSA Training manual data not ship specific : Location / Quantity of equipment , Procedure to use the recovery strops/ recover Rescue boat in rough weather missing","LSA / FFA","Cert. & Docu.","Inappropriate Procedure","5.34","Low","","","-All the LSA/FFA equipments location and quantities inserted against the relevant equipments pages.\n\n-Procedure for recovery of rescue boat in rough weather inserted in the Training Manuals.","2019-09-30","","Completed","2019-09-13","No","No","No","Internal"]
[null,null,null,null,8483,"49_20/12/2019 11:58:37 AM","2019-08-29","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Life jacket markings not in line with SOLAS (\"Front\" missing on all life jackets excluding the oversize and child located in the Fire station. A few of them do not have the standard/ resolution to which they confirm)","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.33","High","","","-Officer incharge immediately marked all lifejackets with FRONT markings.\n\n-Rest all the markings were cross verified with SOLAS standards.","2019-09-30","","Completed","2019-08-30","No","No","No","Internal"]
[null,null,null,null,8484,"49_20/12/2019 12:03:38 PM","2019-08-29","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Helicopter Landing Area markings not in compliance with the IACS guide ","Hull & Tanks","General Appearance","Inappropriate Procedure","11.3","Medium","","","PROPER GUIDELINES HAVE BEEN REFERRED IN IACS GUIDE FOR MARKING IN HELICOPTER LANDING AREA AND CARRIED OUT.","2019-09-30","","Completed","2019-09-13","No","No","No","Internal"]
[null,null,null,null,8485,"49_20/12/2019 12:10:36 PM","2019-08-29","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","VL Load\" marking of the P/S hose saddles and Port side manifold Drp tray capaicty marking missing. ","Miscellaneous","General Appearance","Inappropriate Procedure","9.19","Low","","","THE VL LOAD  AND THE MANIFOLD DRIP TRAY CAPACITY HAS BEEN MARKED.","2019-09-30","","Completed","2019-09-30","No","No","No","Internal"]
[null,null,null,null,5129,"49_27/10/2019 1:56:21 PM","2019-08-30","Defect","Ship Staff","Ship Staff Insp.","AE LT cooler sea water pipe section damaged","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Pipe section renewed","2019-08-30","","Completed","2019-08-30","No","No","No","Internal"]
[null,null,null,null,8455,"49_Mon Oct 28 2019 06:42:17 GMT+0000 (Coordinated Universal Time)","2019-09-11","Defect","Ship Staff","Ship Staff Insp.","AC condenser sea water in andout valves are not holding","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Replaced with new valves","2020-02-25","RESP190150","Completed","2020-02-05","No","No","No","Internal","Will supply during next storing."]
[null,null,null,null,8456,"49_Mon Oct 28 2019 06:43:50 GMT+0000 (Coordinated Universal Time)","2019-09-11","Defect","Ship Staff","Ship Staff Insp.","AE LO purifier speed sensor faulty","E/R - Purifier","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","faulty sensor","2019-11-20","RESP190110","Completed","2019-12-30","No","No","No","Internal"]
[null,null,null,null,5138,"49_27/10/2019 3:38:02 PM","2019-09-11","Defect","Ship Staff","Ship Staff Insp.","Starboard side pilot ladder air motor operating lever not working.","Deck - Machinery","Emgcy. Systems","Equipment Related","9.25","Low","","","Same overhauled and working satisfactory.","2019-09-20","","Completed","2019-09-12","No","No","No","Internal"]
[null,null,null,null,5140,"49_27/10/2019 3:42:02 PM","2019-09-11","Defect","Ship Staff","Ship Staff Insp.","AE3 LT pump oil seal leaky","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.47","Medium","","","Pump overhauled","2019-09-20","","Completed","2019-09-12","No","No","No","Internal"]
[null,null,null,null,8468,"49_Mon Oct 28 2019 06:40:24 GMT+0000 (Coordinated Universal Time)","2019-09-11","Defect","Ship Staff","Ship Staff Insp.","Unit no5 top piston ring broken at butt","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.12","Very High","","","Piston rings were renewed.","2019-11-20","","Completed","2019-11-05","No","No","No","Internal"]
[null,null,null,null,4957,"49_2019-10-28 06:40:24.000","2019-09-11","Defect","Ship Staff","Ship Staff Insp.","Unit no5 top piston ring broken at butt","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.12","Very High","","","UNIT DECARB CARRIED OUT","2019-11-20","","Completed","2019-11-05","No","No","No","Internal","Pls continue to monitor the scavenge temperature & keep this offcie updated."]
[null,null,null,null,4958,"49_2019-10-28 06:42:17.000","2019-09-11","Defect","Ship Staff","Ship Staff Insp.","AC condenser sea water in andout valves are not holding","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Replaced with new valves","2020-02-01","RESP20039","Completed","2020-02-05","No","No","No","Internal",""]
[null,null,null,null,4959,"49_2019-10-28 06:43:50.000","2019-09-11","Defect","Ship Staff","Ship Staff Insp.","AE LO purifier speed sensor faulty","E/R - Purifier","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","sensor renewed and purifier working satisfactory","2019-11-20","","Completed","2019-12-30","No","No","No","Internal","Reference to VFF, RO was cancelled due to Owner arranging supply. Pls advice if you have received the requested spare part, supplied directly by Owner."]
[null,null,null,null,5147,"49_27/10/2019 4:20:28 PM","2019-09-20","Defect","Ship Staff","Ship Staff Insp.","Hydro blaster not building up pressure.","Miscellaneous","General Appearance","Equipment Related","11.1","High","","","All seal are renewed.","2019-09-22","","Completed","2019-09-22","No","No","No","Internal"]
[null,null,null,null,8457,"49_Mon Oct 28 2019 06:45:33 GMT+0000 (Coordinated Universal Time)","2019-09-25","Defect","Ship Staff","Ship Staff Insp.","No2 boiler feed water controller display malfunctioning","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","...","2019-11-20","","Completed","2019-11-30","No","No","No","Internal"]
[null,null,null,null,5145,"49_27/10/2019 4:16:52 PM","2019-09-25","Defect","Ship Staff","Ship Staff Insp.","Main engine T/C grid wash line got choked","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.12","Very High","","","Same cleared","2019-09-30","","Completed","2019-09-29","No","No","No","Internal"]
[null,null,null,null,5146,"49_27/10/2019 4:18:09 PM","2019-09-25","Defect","Ship Staff","Ship Staff Insp.","AE jacket water temp are not maintaining with one jacket cooler in use.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.47","Medium","","","Both AE jacket cooler plates are cleaned","2019-11-20","","Completed","2019-09-25","No","No","No","Internal"]
[null,null,null,null,9285,"49_43766.2816319444","2019-09-25","Defect","Ship Staff","Ship Staff Insp.","No2 boiler feed water controller display malfunctioning","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Dispaly renewed with onboard spare.","2019-11-20","","Completed","2019-12-18","No","No","No","Internal"]
[null,null,null,null,4960,"49_2019-10-28 06:45:33.000","2019-09-25","Defect","Ship Staff","Ship Staff Insp.","No2 boiler feed water controller display malfunctioning","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","controller renewed","2019-11-20","","Completed","2019-12-03","No","No","No","Internal","Have investigation been carried out to verify possible cause of the mulfunction? If yes, pls revert with your findings c/w spares required. If not, when do you plan for same. "]
[null,null,null,null,8458,"49_Mon Oct 28 2019 06:47:14 GMT+0000 (Coordinated Universal Time)","2019-09-26","Defect","Ship Staff","Ship Staff Insp.","IG excess pressure controller not working","Inert Gas","Eng. / Strg. Comp.","Equipment Related","8.33","Medium","","","Rpeated defect","2020-02-01","RESP190167","Completed","2019-09-26","No","No","No","Internal"]
[null,null,null,null,4961,"49_2019-10-28 06:47:14.000","2019-09-26","Defect","Ship Staff","Ship Staff Insp.","IG excess pressure controller not working","Inert Gas","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Controller replaced and found still giving the alarm on controller, pressure sensor out of range. So calibrated to zero and alarm got reset. Check the operation of excess control valve during next operation. ","2020-02-01","RESP200040","Completed","2020-04-16","No","No","No","Internal","RO under processing."]
[null,null,null,null,8486,"49_20/12/2019 12:12:39 PM","2019-10-02","Defect","Ship Staff","Nav Audit / Verification","Procedure for downloading VDR data forgotten/not conversant with some members of the Bridge team as a few members of the Bridge team are relatively new.","Navigation - VDR / BNWAS","Navigation","Human Error","4.11","Medium","","","A VDR Drill has been reconducted and the entire Bridge team has been quizzed post the drill on the procedure to retrieve the data so as to ensure thorough understanding of the same.","2019-10-30","","Completed","2019-10-19","No","No","No","Internal"]
[null,null,null,null,5156,"49_27/10/2019 4:42:10 PM","2019-10-05","Defect","Ship Staff","Ship Staff Insp.","Control air pressure reducing valve leaky","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related","10.47","Medium","","","Same overhauled","2019-10-05","","Completed","2019-10-05","No","No","No","Internal"]
[null,null,null,null,5843,"49_2019-11-03 19:58:03.000","2019-10-05","Defect","Ship Staff","Ship Staff Insp.","ME unit #2, #4aft high pressure pipe leaky","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.12","Very High","","","Same overhauled and leak rectified","2019-10-10","","Completed","2019-10-07","No","No","No","Internal"]
[null,null,null,null,5158,"49_27/10/2019 4:40:24 PM","2019-10-10","Defect","Ship Staff","Ship Staff Insp.","FWG distillate pump discharge line got holed","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.47","Medium","","","Same renewed","2019-10-10","","Completed","2019-10-10","No","No","No","Internal"]
[null,null,null,null,5155,"49_27/10/2019 4:38:59 PM","2019-10-12","Defect","Ship Staff","Ship Staff Insp.","Main engine cylinder head jack leaky","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.12","Very High","","","O ring and back up ring renewed","2019-10-12","","Completed","2019-10-12","No","No","No","Internal"]
[null,null,null,null,8459,"49_Mon Oct 28 2019 06:48:56 GMT+0000 (Coordinated Universal Time)","2019-10-13","Defect","Ship Staff","Ship Staff Insp.","Main engine unit #3 aft and unit #7 both outlet accumulator leaky","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Replaced with newly received spares","2020-11-01","RESP190170","Completed","2020-02-15","No","No","No","Internal"]
[null,null,null,null,5154,"49_27/10/2019 4:37:35 PM","2019-10-13","Defect","Ship Staff","Ship Staff Insp.","Boiler no1 FO tracing steam valve leaky","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Valve renewed","2019-10-15","","Completed","2019-10-16","No","No","No","Internal"]
[null,null,null,null,4962,"49_2019-10-28 06:48:56.000","2019-10-13","Defect","Ship Staff","Ship Staff Insp.","Main engine unit #3 aft and unit #7 both outlet accumulator leaky","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Replaced with newly received spares","2020-01-31","RESP200066","Completed","2020-02-15","No","No","No","Internal","Presume you have made temporary arrangements to control the leaks until requested spares are supplied. Will check with Procurement & advice status of the RO."]
[null,null,null,null,5842,"49_2019-11-03 19:51:10.000","2019-10-14","Defect","Ship Staff","Ship Staff Insp.","Boiler Forward gauge glass leaky","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Leak rectified","2019-10-20","","Completed","2019-10-16","No","No","No","Internal"]
[null,null,null,null,8460,"49_Sun Nov 03 2019 19:55:15 GMT+0000 (Coordinated Universal Time)","2019-10-15","Defect","Ship Staff","Ship Staff Insp.","Hydraulic oil leak in Steering gear compartment.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Repeated defect","2020-01-30","","Completed","2019-10-15","No","No","No","Internal","please plan at first available opportunity"]
[null,null,null,null,8461,"49_Mon Nov 04 2019 18:36:31 GMT+0000 (Coordinated Universal Time)","2019-10-15","Defect","Ship Staff","Ship Staff Insp.","one of the dresser coupling in bunker line leaky","Deck - Pipe / Fittings","Eng. / Strg. Comp.","Equipment Related","8.41","Medium","","","Repition of defect","2020-01-30","RESP190113","Completed","2019-10-15","No","No","No","Internal"]
[null,null,null,null,5844,"49_2019-11-03 20:06:10.000","2019-10-18","Defect","Ship Staff","Ship Staff Insp.","AE Jacket cooler SW pipe section found leaky","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.31","Very High","","","Same rectified","2019-10-20","","Completed","2019-10-19","No","No","No","Internal"]
[null,null,null,null,8469,"49_20/12/2019 7:45:39 AM","2019-11-16","Defect","Ship Staff","Ship Staff Insp.","Atm condenser sea water outlet pipe leak.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","8.11","Medium","","","Pipe leak rectified and inlet and outlet valve which was not holding renewed with new spare.","2019-11-20","","Completed","2019-11-16","No","No","No","Internal"]
[null,null,null,null,8470,"49_20/12/2019 7:50:34 AM","2019-11-17","Breakdown","Ship Staff","Ship Staff Insp.","Sea water service pump no 2 mechanical seal leak","E/R - Aux. Mach.,Miscellaneous","Eng. / Strg. Comp.","Equipment Related","8.11","Medium","","","pump overhauled","2019-11-18","","Completed","2019-11-18","No","No","No","Internal"]
[null,null,null,null,8471,"49_20/12/2019 7:54:05 AM","2019-11-20","Defect","Ship Staff","Ship Staff Insp.","Main cooling sea water pump no 2 mechanical seal leak","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","8.11","Medium","","","pump overhauled","2019-11-21","","Completed","2019-11-21","No","No","No","Internal"]
[null,null,null,null,9996,"49_15-Jan-20 12:43:10 PM","2020-01-01","Critical Equipment","Ship Staff","Ship Staff Insp.","FOAM PUMP MECHANICAL SEAL LEAK","LSA / FFA","Safety / LSA / FFA","Equipment Related","10.32","Very High","","","Mechanical seal renewed.","2020-03-01","resp200030","Completed","2020-09-05","No","No","No","Internal"]
[null,null,null,null,12450,"49_30/04/2020 11:21:01 AM","2020-02-01","Observation","Ship Staff","Ship Staff Insp.","2 No. of Engine room Fire hydrant sfound leaking","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.38","High","","","To be replace","2020-05-01","RESP200104","Completed","2020-04-21","No","No","No","Internal"]
[null,null,null,null,17299,"49_Sat Jan 16 2021 07:53:57 GMT+0000","2020-02-03","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Mechanical Seal of No 1 ballast pump is leaking. To be renewed.","","","","","","","","Mechanical seal replaced and pump tested satisfactory.","2020-05-03","","Completed","2020-03-03","No","No","No","Internal"]
[null,null,null,null,17300,"49_Sat Jan 16 2021 07:56:42 GMT+0000","2020-02-03","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ENGINE BLOWERS COMPARTMENT HAS BECOME DIRTY AND REQUIRED CLEANING","","","","","","","","CLEANED AND PAINTED","2020-05-03","","Completed","2020-04-01","No","No","No","Internal"]
[null,null,null,null,15260,"49_24/11/2020 5:31:10 AM","2020-02-03","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Emergency hand pump of port side hose handling crane was found leaking. Same to be ordered and renewed.","Deck - Machinery","Emgcy. Systems","Equipment Related","8.63","High","","","Seal of port side hose handling crane Emergency hand pump renewed.","2020-05-02","","Completed","2020-04-03","No","No","No","Internal"]
[null,null,null,null,15261,"49_24/11/2020 5:38:23 AM","2020-02-03","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Flange bolts, U clamps and conduit lines forward of mid-ship to be attended","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.3","Medium","","","Completed Derusting and painting of Flange bolts, Uclamps and Conduit line forward of midship.","2020-05-03","","Completed","2020-04-02","No","No","No","Internal"]
[null,null,null,null,15262,"49_24/11/2020 5:53:51 AM","2020-02-03","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Port side on Cargo tank 1 Centre paint is peeling off. Same to be properly blasted and painted.","Hull & Tanks","General Appearance","External Factors","11.3","Medium","","","Port side on Cargo tank 1 Centre properly blasted and painted.","2020-05-03","","Completed","2020-04-20","No","No","No","Internal"]
[null,null,null,null,15263,"49_24/11/2020 6:03:46 AM","2020-02-03","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Railing fwd to manifold area P & S to be blasted and painted.","Hull & Tanks","General Appearance","External Factors","11.3","Medium","","","Railing fwd to manifold area P & S derusted and painted.","2020-05-03","","Completed","2020-04-13","No","No","No","Internal"]
[null,null,null,null,15264,"49_24/11/2020 6:19:17 AM","2020-02-03","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","IG line No.1 and No.2 are in poor condition. to be de rusted and painted.","Deck - Pipe / Fittings","General Appearance","External Factors","11.3","Medium","","","IG line No.1 and No.2 de rusted and painted.","2020-05-03","","Completed","2020-03-21","No","No","No","Internal"]
[null,null,null,null,15265,"49_24/11/2020 6:23:41 AM","2020-02-03","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Hydro blaster is operating at 500 bars. New blaster to be supplied.","Deck - Machinery","General Appearance","Equipment Related","11.1","High","","","New blaster received.","2020-05-03","","Completed","2020-04-15","No","No","No","Internal"]
[null,null,null,null,15266,"49_24/11/2020 6:45:08 AM","2020-02-03","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Provision room does not have suitable baskets. New ones to be ordered. Gratings to be renewed.","Accommodation","General Appearance","Equipment Related","11.1","High","","","New baskets placed in provision store. Gratings renewed.","2020-05-03","","Completed","2020-04-21","No","No","No","Internal"]
[null,null,null,null,15267,"49_24/11/2020 6:48:37 AM","2020-02-03","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Compactor to be relocated as it is fitted in front of the provision rooms.","Accommodation","General Appearance","Equipment Related","11.16","Low","","","Compactor relocated from provision room to Engine room.","2020-11-30","","Completed","2020-11-15","No","No","No","Internal"]
[null,null,null,null,15268,"49_24/11/2020 6:58:10 AM","2020-02-03","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Curtains in Crew mess room to be repaired / renewed as inner lining in poor condition.","Accommodation","General Appearance","Equipment Related","11.16","Low","","","Curtains in Crew mess room repaired / renewed.","2020-05-03","","Completed","2020-04-27","No","No","No","Internal"]
[null,null,null,null,15269,"49_24/11/2020 7:03:51 AM","2020-02-03","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","The crew cabins were found dirty. For AB1 cabin found the flush arrangement is temporary. This is to be rectified.","Accommodation","MLC Related","Equipment Related","11.3","Medium","","","The crew cabins cleaned. For AB1 cabin flush arrangement rectified.","2020-05-03","","Completed","2020-04-25","No","No","No","Internal"]
[null,null,null,null,15270,"49_24/11/2020 7:09:47 AM","2020-02-03","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Treadmill found not working. To be repaired or renewed.","Accommodation","MLC Related","Equipment Related","11.16","Low","","","New Treadmill received and replaced old one.","2020-05-03","","Completed","2020-04-18","No","No","No","Internal"]
[null,null,null,null,15271,"49_24-Nov-20 3:17:34 PM","2020-02-03","Breakdown","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Spare Atmospheric condenser to be cleaned and landed ashore after cleaning ","Cargo Mach.,Elect. Mach. & Equip.,Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.24","Low","","","1 PCS atmospheric condenser witn end covers landed.","2020-09-07","","Completed","2020-08-20","No","No","No","Internal"]
[null,null,null,null,15272,"49_24-Nov-20 3:32:03 PM","2020-02-03","Other","Owner / Marine / Tech. Suptd.","Ship Staff Insp.","E/R log book found not filled up. ME FO Cons/UMS alarms/LO Cons/ BWT-CWT tests. Daily running hour not logged","Miscellaneous","Cert. & Docu.","Human Error","2.9","Medium","","","Instuction given to all the engineers to write down all data as per requirment.","2020-03-08","","Completed","2020-02-07","No","No","No","Internal"]
[null,null,null,null,15273,"49_24-Nov-20 3:40:48 PM","2020-02-03","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Leak Noticed at FWD end of the main engine casing to be rectified.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.12","Very High","","","Leak rectified and kept under observation found good.","2020-03-06","","Completed","2020-03-01","No","No","No","Internal"]
[null,null,null,null,15276,"49_24/11/2020 6:00:58 AM","2020-02-03","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Cover of windlass is in poor condition. Same to be repaired.","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.3","Medium","","","Job added in Refman. To be done in Dry dock.","2021-02-28","","Completed","2020-11-06","No","No","No","Internal"]
[null,null,null,null,15277,"49_24/11/2020 7:07:18 AM","2020-02-03","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Crew mess room AC duct louvers are missing. New ones to be ordered and installed.","Accommodation","MLC Related","Equipment Related","11.16","Low","","","Crew mess room AC duct louvers renewed.","2020-05-03","","Completed","2020-04-18","No","No","No","Internal"]
[null,null,null,null,15278,"49_24/11/2020 6:14:19 AM","2020-02-03","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","10 Nos of Hydraulic boxes covers to be repaired and blasted and painted with two coats of Epoxy paint.","Deck - Pipe / Fittings","General Appearance","External Factors","11.1","High","","","Hydraulic boxes covers blasted and painted with two coats of Epoxy paint. Renewal of box covers to be done in Dry dock.","2021-02-28","","Completed","2020-11-06","No","No","No","Internal"]
[null,null,null,null,15279,"49_24-Nov-20 3:07:09 PM","2020-02-03","Breakdown,Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Flash back arrestor on Oxygen and Acetylene room to be renewed.","Miscellaneous","Safety / LSA / FFA","Equipment Related","5.27","Medium","","","Flash back arrestor renewed.","2020-04-08","","Completed","2020-03-05","No","No","No","Internal"]
[null,null,null,null,12453,"49_07/05/2020 11:49:08 AM","2020-02-05","Observation","Ship Staff","ISM Audit","Lifeboat seat belts were not in alternate colours","LSA / FFA","Safety / LSA / FFA","Human Error","5.29","High","","","Seat belts renewed and confirmed in alternate colours","2020-02-05","RESP205015","Completed","2020-02-06","No","No","No","Internal"]
[null,null,null,null,12418,"49_02/03/2020 08:47:42","2020-02-07","Defect","Ship Staff","Ship Staff Insp.","Main engine unit 7 cooling water leakage from cylinder cover","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Onboard spare new cylinder head (2 Pcs) are not suitable for use as opening for injector nozzle is small not allowing injectors to be installed properly.Supplied by owner. Communication in progress.Job added to refman, will be done in drydock.","2021-02-28","RESP 200033","Completed","2020-11-24","No","No","No","Internal"]
[null,null,null,null,12424,"49_28-Feb-20 5:36:22 PM","2020-02-07","Defect","Ship Staff","Ship Staff Insp.","Steering gear unit 3 servo pump oil seal leakage ","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Oil seal to be renewed. Job has been transfered to refman. Job will be done in drydock.","2021-02-28","RESP 200117","Completed","2020-11-24","No","No","No","Internal"]
[null,null,null,null,12432,"49_17/2/2020 8:53:59 AM","2020-02-07","Observation","Ship Staff","Ship Staff Insp.","Safety walkway steps found with holes or almost broken due to corrosion.","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","Equipment Related","11.1","High","","","Soft repairs carried out on areas of minor corrosion. New steps to be fabricated and fitted where substantial corrosion or damage has occured.","2020-03-15","","Completed","2020-03-06","No","No","No","Internal"]
[null,null,null,null,12439,"49_26-Feb-20 3:01:44 PM","2020-02-07","Defect","Ship Staff","Ship Staff Insp.","MGPS not in use as anodes depleted,anodes not renewed as valves not holding","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Lines to the MGPS blanked and anodes renewed. Blanks removed and system inspected and put into use","2020-04-01","","Completed","2020-04-10","No","No","No","Internal"]
[null,null,null,null,12459,"49_28-Feb-20 12:49:03 AM","2020-02-07","Defect","Ship Staff","Ship Staff Insp.","Intermediate shaft oil slinger leakage","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Oil slinger removed and fitted with newly received spares.","2020-04-07","RESP 200118","Completed","2020-05-27","No","No","No","Internal"]
[null,null,null,null,12427,"49_02/03/2020 08:56:29","2020-02-10","Defect","Ship Staff","Ship Staff Insp.","Fresh water generator condenser leaking from end cover ","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.47","Medium","","","End cover removed and packing renewed","2020-03-30","","Completed","2020-03-03","No","No","No","Internal"]
[null,null,null,null,12428,"49_02/03/2020 08:59:54","2020-02-10","Defect","Ship Staff","Ship Staff Insp.","Main engine jacket water heater leakage from tube end gasket","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.47","Medium","","","Tube end gasket to renewed after isolating the system completely.","2020-03-30","","Completed","2020-03-07","No","No","No","Internal"]
[null,null,null,null,12433,"49_02/03/2020 08:53:38","2020-02-10","Defect","Ship Staff","Ship Staff Insp.","Air ejector condesser leakage from end cover packing","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.31","Very High","","","Steam and cooling sea water valve renewed, overhauled. Condenser end cover opened, tube cleaned and cover packing renewed","2020-04-30","","Completed","2020-03-14","No","No","No","Internal"]
[null,null,null,null,4923,"49_24/10/2019 5:11:04 AM","2020-02-12","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Accommodation block front , port, stbd, and aft to be derusted and painted.","Accommodation","General Appearance","External Factors","11.8","Low","","","Derusting and painting of front completed. De-rusting of port and stbd bridge wing support pillars completed. De-rusting & painting of A-deck & B-deck port side completed. Aft accommodation area derusting and painting completed","2020-02-28","","Completed","2020-02-12","No","No","No","Internal",""]
[null,null,null,null,12429,"49_07/03/2020 08:44:58","2020-02-20","Defect","Ship Staff","Ship Staff Insp.","Air ejector steam inlet valve leaky, not holding.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.14","Medium","","","Main steam isolated and one new valve fitted and other lapped and fitted back","2020-03-30","","Completed","2020-03-06","No","No","No","Internal"]
[null,null,null,null,12430,"49_07/03/2020 08:47:58","2020-02-20","Defect","Ship Staff","Ship Staff Insp.","Steam valve for the overflow tank not holding.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.14","Medium","","","Main steam isolated and new valve fitted","2020-03-30","","Completed","2020-03-06","No","No","No","Internal"]
[null,null,null,null,12431,"49_13/03/2020 08:11:35","2020-02-20","Defect","Ship Staff","Ship Staff Insp.","Main engine lube oil storage tank spring loaded drain valve leakage","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.14","Medium","","","Valve inspected and found gland in bad shape, o ring fitted alogn with the gland to arrest the leakage","2020-04-20","","Completed","2020-03-12","No","No","No","Internal"]
[null,null,null,null,12434,"49_07/03/2020 08:42:43","2020-02-20","Defect","Ship Staff","Ship Staff Insp.","Steam dump valve to the vacuum condesner leaking and condenser getting hot","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.14","Medium","","","Main steam isolated and valve replaced with overhauled one.","2020-03-30","","Completed","2020-03-06","No","No","No","Internal"]
[null,null,null,null,12452,"49_07/05/2020 8:53:36 PM","2020-02-26","Defect","Ship Staff","Ship Staff Insp.","3 NOS OF FOAM MONITOR VALVES FOUND LEAKING.","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.38","High","","","VALVES RENEWED WITH RECEIVED SPARES","2020-03-26","RESP200112","Completed","2020-03-24","No","No","No","Internal"]
[null,null,null,null,12449,"49_07/05/2020 8:48:03 PM","2020-02-27","Defect","Ship Staff","Ship Staff Insp.","DURING MONTHLY INSPECTION 3 NOS OF LIFEBUOY FOUND CRACKED.","LSA / FFA","Safety / LSA / FFA","Behaviour Based","5.31","High","","","LIFEBUOYS RENEWED WITH AVAILABLE SPARES","2020-03-10","","Completed","2020-02-29","No","No","No","Internal"]
[null,null,null,null,12444,"49_30/04/2020 11:28:25 AM","2020-03-01","Defect","Ship Staff","Ship Staff Insp.","Stbd Side Lifeboat entrance door hatch found damaged","LSA / FFA","Safety / LSA / FFA","Behaviour Based,Human Error","5.29","High","","","To be repaired with repair kit","2020-05-01","RESP200115","Completed","2020-04-24","No","No","No","Internal"]
[null,null,null,null,12435,"49_07/03/2020 08:52:09","2020-03-02","Defect","Ship Staff","Ship Staff Insp.","FWG and deck seal pump 2 seal leakage","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.31","Very High","","","Pump opened up and inspected, found mechanical seal damaged. Fitted with new mechanical seal and leakage arrested.","2020-04-30","","Completed","2020-03-14","No","No","No","Internal"]
[null,null,null,null,12437,"49_07/03/2020 08:54:28","2020-03-02","Defect","Ship Staff","Ship Staff Insp.","Observation tank sight glass not clear, top cover packing damaged and leaking.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.14","Medium","","","Observation tank cover opened and inspected, sight glass cleaned and gasket renewed","2020-04-30","","Completed","2020-03-07","No","No","No","Internal"]
[null,null,null,null,12419,"49_14/3/2020 2:49:27 PM","2020-03-09","Defect","Ship Staff","Ship Staff Insp.","Oxygen sensors of VECS manifolds are non-operational. ","Inert Gas","Cargo / Ballast Systems","Equipment Related","8.42","Medium","","","Need guidance for installing new transmitter as connections are different from the one in use.Awaiting reply from Mr kamlesh solanki. Communication in progress. Job added in Refman. To be done in Drydock.","2021-02-28","RESP200050 ","Completed","2020-11-06","No","No","No","Internal"]
[null,null,null,null,12438,"49_13/03/2020 08:16:27","2020-03-09","Defect","Ship Staff","Ship Staff Insp.","Main engine jacket water cooler sea water inlet pipe has corrosion damage resulting in pin hole","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.31","Very High","","","Pipe fabricated and damaged pipe replaced","2020-03-30","","Completed","2020-03-17","No","No","No","Internal"]
[null,null,null,null,12448,"49_07/05/2020 11:44:36 AM","2020-03-15","Observation","Ship Staff","Ship Staff Insp.","Gripe Lashing wire for Port Lifeboat found in poor condition during inspection","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.29","High","","","Gripe Lashing renewed","2020-04-15","","Completed","2020-03-31","No","No","No","Internal"]
[null,null,null,null,12425,"49_27-Mar-20 3:38:55 PM","2020-03-18","Defect","Ship Staff","Ship Staff Insp.","Aux engine 3 centrifuge filter not working as the body is damaged beyond repair","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Spares received , Filter body renewed and system made opearational.","2020-05-18","","Completed","2020-09-01","No","No","No","Internal"]
[null,null,null,null,12436,"49_22-Mar-20 9:59:40 AM","2020-03-18","Defect","Ship Staff","Ship Staff Insp.","Fresh water hydrophore inlet valve, hydrophore pump 1 inlet and outlet valve not holding ","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.3","Medium","","","System isolated and valves removed, replaced or renewed with new valves","2020-03-31","","Completed","2020-03-22","No","No","No","Internal"]
[null,null,null,null,12443,"49_27-Mar-20 3:42:31 PM","2020-03-22","Defect","Ship Staff","Ship Staff Insp.","Fire and bilge pump discharge line has corrosion damage resulting leakage ","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.31","Very High","","","Pipe removed from place and repaired ","2020-04-22","","Completed","2020-04-29","No","No","No","Internal"]
[null,null,null,null,12451,"49_2/4/2020 9:54:34 AM","2020-04-02","Observation","Ship Staff","Ship Staff Insp.","Lifeboat remote lowering wire was found in poor condiiton due to corrosion, wear and tear.","LSA / FFA","Safety / LSA / FFA","Equipment Related,External Factors","5.29","High","","","Wires renwed with spares received","2020-06-02","RESP200115","Completed","2020-05-08","No","No","No","Internal"]
[null,null,null,null,12445,"49_1/5/2020 8:39:36 PM","2020-04-05","Observation","Class Surveyor","OM Insp. (Eg. SIRE / CDI etc.)","CLC wreck removal could not be located at the time of inspection","Documentation","Cert. & Docu.","Human Error","2.1","Very High","","","A scanned copy was made available onboard prior completion of inspection","2020-04-05","","Completed","2020-04-05","No","No","No","External"]
[null,null,null,null,12446,"49_1/5/2020 8:44:33 PM","2020-04-05","Observation","Class Surveyor","OM Insp. (Eg. SIRE / CDI etc.)","The maintenance and operation instructions was not present in the SOLAS training manual presented","Documentation","ISM Related","Human Error","5.34","Low","","","The SOLAS training manual was updated with maintenance and operations instructions before the completion of inspection","2020-04-05","","Completed","2020-04-05","No","No","No","External"]
[null,null,null,null,12447,"49_1/5/2020 8:47:28 PM","2020-04-05","Observation","Class Surveyor","OM Insp. (Eg. SIRE / CDI etc.)","No3 AUX engine was noted with lubrication oil leak from lub oil pump","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","The leak was rectified prior completion of inspection","2020-04-05","","Completed","2020-04-05","No","No","No","External"]
[null,null,null,null,12460,"49_16/4/2020 2:05:20 PM","2020-04-14","Defect","Ship Staff","Ship Staff Insp.","During STS mooring operations, minor leak was observed from connections of M2 mooring winch.","Deck - Mooring Machinery","Mooring","Equipment Related","9.14","Medium","","","Winch to be isolated. Damaged part taken to ER workshop and repairs carried out.","2020-05-14","","Completed","2020-05-08","No","No","No","Internal"]
[null,null,null,null,12420,"49_1/5/2020 8:56:45 PM","2020-04-15","Observation","Class Surveyor","OM Insp. (Eg. SIRE / CDI etc.)","Vessel hull topside heavily discoloured with corrosion over 40% of the visible area. Boot top area with exposed undergrowth and moderate marine growth for the entire length of vessel.","Hull & Tanks","General Appearance","External Factors","11.1","High","","","Job added to refman. Job deferred to Dry Dock","2021-02-28","","Completed","2020-11-06","No","No","No","External"]
[null,null,null,null,12421,"49_1/5/2020 9:02:01 PM","2020-04-15","Observation","Class Surveyor","OM Insp. (Eg. SIRE / CDI etc.)","Weather decks with over 30% spot rust and seepage. Maintenance was in progress with visible improvment in bow and poop areas.","Hull & Tanks","General Appearance","External Factors","11.3","Medium","","","Derusting and painting completed with hydroblaster with priority for areas with maximum spot rust density.","2020-08-15","","Completed","2020-11-21","No","No","No","External"]
[null,null,null,null,12442,"49_18-Apr-20 11:44:37 AM","2020-04-15","Defect","Ship Staff","Ship Staff Insp."," Air leakage from the valve block of inert gas system. ","Inert Gas","Cargo / Ballast Systems","Equipment Related","10.32","Very High","","","Air leakage was caused by the non operating air seal valve for 2 aux boiler which were rectified ","2020-04-30","","Completed","2020-04-20","No","No","No","Internal"]
[null,null,null,null,12454,"49_28/4/2020 8:34:37 PM","2020-04-15","Defect","Ship Staff","Ship Staff Insp.","During routine rounds M3 mooring winch outboard hydraulic motor seal was found to be leaking.","Deck - Mooring Machinery","Mooring","Equipment Related","9.14","Medium","","","Hydraulic motor removed from place and oil seal renewed, fitted back and tried out.","2020-05-20","","Completed","2020-05-08","No","No","No","Internal"]
[null,null,null,null,12461,"49_28/4/2020 8:44:23 PM","2020-04-15","Defect","Ship Staff","Ship Staff Insp.","Gas discharge pipeline from AUS to Slop Port tank very badly corroded and holed. ","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.8","Medium","","","Lines are removed section-wise taken to ER for repairs. Derusted, 2 primer and top coat painted. 3 sections completed. ","2020-05-15","","Completed","2020-05-15","No","No","No","Internal"]
[null,null,null,null,12440,"49_18-Apr-20 11:50:35 AM","2020-04-17","Observation","Owner / Marine / Tech. Suptd.","Bunkering Audit","Bunker safety checklist Code \"A\" to be signed by both parties.","Documentation","Eng. / Strg. Comp.","Human Error","10.1","Medium","","","All the safety checklist checked and corrected ","2020-04-30","","Completed","2020-04-18","No","No","No","Internal"]
[null,null,null,null,12441,"49_18-Apr-20 11:53:40 AM","2020-04-17","Observation","Owner / Marine / Tech. Suptd.","Bunkering Audit","12.04.08.011.02 Bunker transferring plan - Post bunkering checklist completion time not recorded.","Documentation","Eng. / Strg. Comp.","Human Error","10.1","Medium","","","12.04.08.011.02 Bunker transferring plan - Post bunkering checklist completion time recorded.","2020-04-30","","Completed","2020-04-18","No","No","No","Internal"]
[null,null,null,null,null,"49_28/4/2021 11:11:25 AM","2020-04-17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Pump room flap indicators are wasted. ","Cargo Mach.","Emgcy. Systems","Equipment Related",5.45,"Medium","Not Applicable","Not Applicable","Wasted lever renewed","2021-05-31",null,"Completed","2021-05-22","No",null,null,"Internal"]
[null,null,null,null,12457,"49_30-Apr-20 12:58:14 PM","2020-04-29","Defect","Ship Staff","Ship Staff Insp.","Main engine unit 7 shock absorber leaking.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Shock absorber removed, overhauled and fitted back","2020-05-30","","Completed","2020-05-28","No","No","No","Internal"]
[null,null,null,null,12456,"49_04/05/2020 3:38:23 PM","2020-05-02","Defect","Ship Staff","Ship Staff Insp.","Shaft earthing potential is high. Cleaned the slip terminal,contacts ,brush etc still not decreasing. Suspecting corrosion between the slip ring and shaft","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Slip ring removed from place and contact surface of shaft thoroughly cleaned, also the slip ring surface cleaned and fitted back.","2020-07-30","","Completed","2020-05-27","No","No","No","Internal"]
[null,null,null,null,12455,"49_27-May-20 10:50:09 PM","2020-05-12","Defect","Ship Staff","Ship Staff Insp.","Main engine unit #4 exhaust valve sealing air unit leaking and creating fine spray of oil","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Sealing air blcok covered with felt filter, later the sealing unit removed and overhauled. O rings found to be damaged and which were replaced.","2020-05-31","","Completed","2020-05-22","No","No","No","Internal"]
[null,null,null,null,13601,"49_13/07/2020 6:52:04 PM","2020-05-15","Breakdown","Ship Staff","Ship Staff Insp.","Weather Facsimile Receiver (Model- JRC JAX-9A) is inoperational and “Battery Failure” alarm was displyed. \n\n","Navigation - GMDSS & Communication","Communication","Equipment Related","4.19","Low","","","Renewed complete set tried out found working in good order","2020-07-31","","Completed","2020-09-07","No","No","No","Internal"]
[null,null,null,null,13610,"49_23-Jun-20 7:47:31 PM","2020-06-17","Defect","Ship Staff","Ship Staff Insp.","Main engine unit 5 cylinder liner cooling water inlet pipe leaking","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","4 Cooling water pipes removed and o ring renewed","2020-08-30","","Completed","2020-06-24","No","No","No","Internal"]
[null,null,null,null,13616,"49_04-Jul-20 10:13:46 PM","2020-07-02","Defect","Ship Staff","Ship Staff Insp.","EPC-50 card for HFO purifier is faulty and needs to be renewed.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","New spare EPC 50 card received same replaced with old one.","2020-08-30","","Completed","2020-08-29","No","No","No","Internal"]
[null,null,null,null,13612,"49_13/7/2020 9:24:03 AM","2020-07-03","Defect","Ship Staff","Ship Staff Insp.","During heavy weather, due to strong winds, spray and vibration, one deck light on fwd mast broke from foundation.","Elect. Mach. & Equip.","General Appearance","External Factors","11.9","Low","","","The foundation was removed taken to ER for repairs, painted and fixed back.","2020-07-26","","Completed","2020-07-21","No","No","No","Internal"]
[null,null,null,null,13602,"49_14/07/2020 5:06:24 AM","2020-07-04","Defect","Ship Staff","Ship Staff Insp.","Stbd and port gangway pneumatic line U-clamps, supports and air filter boxes corroded and broken.","Deck - Pipe / Fittings","General Appearance","External Factors","11.4","Very High","","","Repair and fabrication of supports, U-clamps and boxes to be carried out. Port side ganway one box renewed. Job added in Refman to be done in dry dock.","2021-02-28","","Completed","2020-11-06","No","No","No","Internal"]
[null,null,null,null,13614,"49_29-Jul-20 10:32:28 AM","2020-07-19","Defect","Ship Staff","Ship Staff Insp.","Stern tube forward seal temperature increased and also the leakage from seal increased","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","S/T FWD seal renewed by the technicians.","2020-08-30","","Completed","2020-08-28","No","No","No","Internal"]
[null,null,null,null,13606,"49_30/7/2020 12:10:45 AM","2020-07-20","Observation","Ship Staff","Ship Staff Insp.","Stbd drip tray fwd access ladder steps corroded. Need to be renewed","Miscellaneous","General Appearance","External Factors","11.3","Medium","","","Added in Refman for renewal at Drydock.","2021-02-28","","Completed","2020-11-06","No","No","No","Internal"]
[null,null,null,null,13603,"49_14/07/2020 5:10:30 AM","2020-08-27","Defect","Ship Staff","Suptd. Insp.","Port and stbd manifold electrical line supports and ESD button supports corroded and broken.","Deck - Pipe / Fittings","General Appearance","","11.4","Very High","","","Renewal/ repairs to be carried out. Port /\\Stbd side all angle bar supports renewed.","2020-11-27","","Completed","2020-11-06","No","No","No","Internal"]
[null,null,null,null,13611,"49_23-Jun-20 7:56:10 PM","2020-08-27","Defect","Ship Staff","Suptd. Insp.","Main engine jacket cooling water pump 2 mechanical seal found leaking","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Pump overhauled and seal renewed","2020-09-07","","Completed","2020-08-31","No","No","No","Internal"]
[null,null,null,null,13613,"49_29/7/2020 11:49:56 PM","2020-08-27","Breakdown","Ship Staff","Suptd. Insp.","Bridge central wiper  not operational.","Navigation - Others","Navigation","Equipment Related","4.3","Medium","","","Wiper to be removed from location, investigated. Broken wheel repaired. Wiper tried out.","2020-10-31","","Completed","2020-09-10","No","No","No","Internal"]
[null,null,null,null,13615,"49_06-Aug-20 11:08:06 AM","2020-08-27","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Fuel oil circulating pump stand by start pressure switch defective.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","renwed pressure switch","2020-10-06","RESP200234","Completed","2020-08-31","No","No","No","Internal"]
[null,null,null,null,14658,"49_18/09/2020 10:26:39","2020-08-27","Defect","Ship Staff","Suptd. Insp.","Hot water calorifier electric heater found in operational,  To be rectified","Accommodation","Eng. / Strg. Comp.","Equipment Related","10.3","Medium","","","Insulation resistance checked, found zero. Electrical heater renewed from spare,","2020-11-30","","Completed","2020-10-18","No","No","No","Internal",""]
[null,null,null,null,14661,"49_18/09/2020 10:46:30","2020-08-27","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","MGPS anodes current low with no Spares onboard.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","New spares received, installed and system made operational.","2020-11-30","","Completed","2020-11-27","No","No","No","Internal",""]
[null,null,null,null,14663,"49_02/09/2020 11:47:55","2020-08-27","Defect","Ship Staff","Suptd. Insp.","Observed air leak from operating air cylinder for funnel flaps.","LSA / FFA","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Air cylinder seal renewed, leak rectified, system operation checked, all found in good working order.","2020-09-05","","Completed","2020-09-01","No","No","No","Internal"]
[null,null,null,null,17298,"49_Sat Jan 16 2021 07:48:40 GMT+0000","2020-08-27","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Galley Fridge not working","","","","","","","","Rectified and working","2020-11-27","","Completed","2020-09-30","No","No","No","Internal"]
[null,null,null,null,15251,"49_24/11/2020 5:48:43 AM","2020-08-27","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Main deck Cargo Tank 2 Wings & 3 Wings area to be reblasted and painted.","Hull & Tanks","General Appearance","External Factors","11.3","Medium","","","Main deck Cargo Tank 2 Wings & 3 Wings area reblasted and painted.","2021-02-01","","Completed","2020-11-17","No","No","No","Internal",""]
[null,null,null,null,15252,"49_17-Nov-20 2:23:15 PM","2020-08-27","Defect","Ship Staff","Suptd. Insp.","Hospital sanitary exhaust fan found defective","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.3","Medium","","","Renewed","2020-11-27","","Completed","2020-10-28","No","No","No","Internal",""]
[null,null,null,null,15255,"49_24/11/2020 6:07:52 AM","2020-08-27","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Stbd manifold area to be re blasted and painted.","Hull & Tanks","General Appearance","External Factors","11.4","Very High","","","Stbd manifold area  re blasted and painted.","2020-11-27","","Completed","2020-11-18","No","No","No","Internal",""]
[null,null,null,null,12458,"49_12/05/2020 10:52:47 PM","2020-08-27","Defect,Observation","Ship Staff","Suptd. Insp.","Lashing and Fastening Gripes for Stbd Lifeboat found in poor condition.","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.29","High","","","Wires renewed.","2020-09-05","","Completed","2020-08-31","No","No","No","Internal"]
[null,null,null,null,15274,"49_24/11/2020 5:22:04 AM","2020-08-27","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Coaming of pumproom blowers to be repaired.","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","Equipment Related","11.4","Very High","","","Added in Refman. To be done in Dry dock.","2020-11-27","","Completed","2020-11-06","No","No","No","Internal","Added in DD Specs"]
[null,null,null,null,15280,"49_24/11/2020 6:53:27 AM","2020-08-27","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Port holes in officer Mess room 2 Nos, Galley 1 no., Crew mess room 3 Nos. are leaking. To be rectified.","Accommodation","Structural Condn. / WT integrity ","External Factors","11.16","Low","","","Job enetered in Refman. To be rectified in Dry dock.","2020-11-27","","Completed","2020-10-27","No","No","No","Internal"]
[null,null,null,null,13600,"49_04-Jul-20 10:17:17 PM","2020-11-02","Defect","Ship Staff","Ship Staff Insp.","Incinerator operating panel defective and triggers alarm and shut down of incinerator frequently","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Replaced Operating panel and main programable module , tried out found working in good order.","2020-12-31","","Completed","2020-12-16","No","No","No","Internal"]
[null,null,null,null,15256,"49_20/11/2020 6:40:01 PM","2020-11-04","Defect","Ship Staff","Ship Staff Insp.","course recorder rotating motor not working","Navigation - Others","Navigation","Equipment Related","4.19","Low","","","Technician attended and did maintenace now system is operational","2020-12-25","","Completed","2020-12-14","No","No","No","Internal"]
[null,null,null,null,12422,"49_1/5/2020 9:09:20 PM","2020-11-15","Observation","Class Surveyor","OM Insp. (Eg. SIRE / CDI etc.)","WBT 1S,5P & 5S observed from deck. Ladder rungs were moderately corroded. 1st platform with heavy spot corrosion over 40% of visible area. Longitudnals with 30% corrosion on edges","Hull & Tanks","Structural Condn. / WT integrity ","External Factors","2.16","Medium","","","Thinned down ladder and plated renewed in Drydock.","2021-03-30","","Completed","2021-04-16","Yes","No","No","External","Job will be carried out during vessel docking."]
[null,null,null,null,15258,"49_20/11/2020 6:47:52 PM","2020-11-15","Defect","Ship Staff","Ship Staff Insp.","ECDIS NO - 1 UPS Malfunctioning","Navigation - ECDIS","Navigation","Equipment Related","4.19","Low","","","Renewed UPS and tried out working in good order","2021-02-15","","Completed","2020-12-15","No","No","No","Internal","RO in processing stage."]
[null,null,null,null,13605,"49_18/07/2020 12:50:25 PM","2020-11-18","Defect","Ship Staff","Ship Staff Insp.","Main cooling sea water pump 2 mechanical seal leakaing","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Seal to be renwed during ballast passage.","2020-11-30","","Completed","2020-11-16","No","No","No","Internal",""]
[null,null,null,null,12426,"49_30-Apr-20 6:40:38 PM","2020-11-19","Defect","Ship Staff","Ship Staff Insp.","Port side uppder deck speaker for public address system defective.","Elect. Mach. & Equip.","Communication","Equipment Related","5.35","Medium","","","Replaced with new one tested found satisfactory.","2020-12-31","","Completed","2020-12-15","No","No","No","Internal","Order currently with K&N Osaka."]
[null,null,null,null,13609,"49_31/08/2020 13:41:25","2020-11-24","Breakdown","Ship Staff","Ship Staff Insp.","Lube oil prifier EPC 50 card malfunctioning and needs to be renewed.","E/R - Purifier","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","EPC 50 card  renewed after receipt of spares","2021-02-28","","Completed","2021-02-16","No","No","No","Internal","Spares connected to vsl."]
[null,null,null,null,18881,"49_28/4/2021 3:25:39 PM","2021-03-20","Observation","Ship Staff","Ship Staff Insp.","EGB Safety valve found leaking","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","EGB safety valve overhauled and pressure tested by yard during drydocking","2021-04-08","","Completed","2021-04-08","No","No","No","Internal"]
[null,null,null,null,18862,"49_28/4/2021 11:21:41 AM","2021-04-17","Critical Equipment,Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","All identified Leakages in the valve hydraulic system to be repaired.","Deck - Machinery","Cargo / Ballast Systems","Equipment Related","8.11","Medium","","","All leaks rectified.","2021-05-02","","Completed","2021-05-01","No","No","No","Internal"]
[null,null,null,null,18864,"49_28/4/2021 11:42:44 AM","2021-04-17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Fwd Mast Stay wire missing. To be installed","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.8","Low","","","New stay wire  installed.","2021-05-02","","Completed","2021-05-01","No","No","No","Internal"]
[null,null,null,null,18882,"49_28/4/2021 11:25:47 AM","2021-04-17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Leak on the port side windlass hydraulic motor to be rectified","Deck - Mooring Machinery","Mooring","Equipment Related","","","","","Hydraulic motor removed and oil seal renewed and bearing cover plate housing renewed","2021-05-02","","Completed","2021-04-20","No","No","No","Internal"]
[null,null,null,null,18883,"49_28/4/2021 11:31:06 AM","2021-04-17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Port side hose handling crane return line block O rings to be renewed.","Deck - Machinery","Cargo / Ballast Systems","Equipment Related","","","","","Block O-ring /Hydraulic rotary coupling renewed by GMTSS technicians and crane tested for operation. Load test also carried out.","2021-05-02","","Completed","2021-04-20","No","No","No","Internal"]
[null,null,null,null,null,"49_28/4/2021 12:15:39 PM","2021-04-17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","E/R Bilges to be cleaned","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Bilge wells cleaned","2021-05-17",null,"Completed","2021-05-10","No",null,null,"Internal"]
[null,null,null,null,null,"49_28/4/2021 12:26:26 PM","2021-04-17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Leaking SW pipe on the AE Plate cooler to be renewed.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related",10.29,"Medium","Not Applicable","Not Applicable","pipe section removed and repaired in E/R workshop","2021-05-17",null,"Completed","2021-05-17","No",null,null,"Internal"]
[null,null,null,null,null,"49_28/4/2021 12:23:30 PM","2021-04-17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Cylinder oil tank gauging system not working. The float to be fixed with the newly procured wire.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","New wire and float installed. System adjusted for correct sounding. Showing correct reading","2021-05-17",null,"Completed","2021-05-14","No",null,null,"Internal"]
[null,null,null,null,null,"49_28/4/2021 12:30:21 PM","2021-04-17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Economiser feed pump NO 1 not working. To be renewed with the new one supplied.  ","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","pump overhauled with all available spares onboard. Pump tried out, found working satisfactory","2021-05-31",null,"Completed","2021-05-07","No",null,null,"Internal"]
[null,null,null,null,null,"49_28/4/2021 2:56:27 PM","2021-04-17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","No3 Vent fan motor could not be overhauled during docking repairs. Same  to be overhauled at first opportunity.","E/R - Aux. Mach.,Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related",10.37,"Medium","Not Applicable","Not Applicable","No 3 vent fan motor removed and overhauled with new bearings","2021-07-17",null,"Completed","2021-05-17","No",null,null,"Internal"]
[null,null,null,null,null,"49_28/4/2021 3:10:19 PM","2021-04-17","Observation","Owner / Marine / Tech. Suptd.","Ship Staff Insp.","ECR found dirty. Bulkheads to be cleaned and posters to be removed from the bulkheads and posted on the felt notice boards.","Miscellaneous","General Appearance","Knowledge Based",10.29,"Medium","Not Applicable","Not Applicable","ECR cleaned, all unwanted posters removed, bulkhead cleaned","2021-05-16",null,"Completed","2021-05-11","No",null,null,"Internal"]
[null,null,null,null,null,"49_28/4/2021 12:20:34 PM","2021-04-17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Many pressure gauges were found defective on the engine room pumps. New gauges have been supplied These are to be renewed. ","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Various pressure gauges renewed","2021-05-17",null,"Completed","2021-05-08","No",null,null,"Internal"]
[null,null,null,null,null,"49_28/4/2021 11:18:49 AM","2021-04-17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Pump room dirty. To be cleaned.","Miscellaneous","General Appearance","Equipment Related",11.3,"Medium","Not Applicable","Not Applicable","Pump room cleaned","2021-05-16",null,"Completed","2021-05-12","No",null,null,"Internal"]
[null,null,null,null,null,"49_28/4/2021 11:56:20 AM","2021-04-18","Observation","Ship Staff","Ship Staff Insp.","Cargo manifold spill tray drain valves to COT 4P & 4S badly corroded","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related",8.11,"Medium","Not Applicable","Not Applicable","Both valves valves renewed","2021-05-17",null,"Completed","2021-05-15","No",null,null,"Internal"]
[null,null,null,null,null,"49_28/4/2021 11:53:33 AM","2021-04-18","Observation","Ship Staff","Ship Staff Insp.","Hydraulic return line for mooring winch/windlass near no.6 foam monitor leaking","Deck - Mooring Machinery","Mooring","Equipment Related",9.14,"Medium","Not Applicable","Not Applicable","New pipe section fabricated and renewed with new gaskets","2021-05-17",null,"Completed","2021-05-17","No",null,null,"Internal"]
[null,null,null,null,null,"49_28/4/2021 11:51:49 AM","2021-04-18","Observation","Ship Staff","Ship Staff Insp.","Hydraulic return line for M3 mooring winch leaking","Deck - Mooring Machinery","Mooring","Equipment Related",9.14,"Medium","Not Applicable","Not Applicable","New pipe section fabricated and renewed with new gaskets","2021-05-17",null,"Completed","2021-05-08","No",null,null,"Internal"]
[null,null,null,null,null,"49_28/4/2021 11:49:28 AM","2021-04-18","Observation","Ship Staff","Ship Staff Insp.","Leak observed in high pressure pipe of valve control block of stbd windlass","Deck - Machinery","Mooring","Equipment Related",9.1999999999999993,"Very High","Not Applicable","Not Applicable","New pipe section fabricated and renewed","2021-05-17",null,"Completed","2021-05-12","No",null,null,"Internal"]
[null,null,null,null,null,"49_04/06/2021 12:48:12 PM","2021-05-02","Observation","Ship Staff","Ship Staff Insp.","Mooring winch/windlass hydraulic line casing return valves leaking (3 nos.)","Deck - Mooring Machinery","Mooring","Equipment Related",9.14,"Medium","Not Applicable","Not Applicable","All 3 casing return valves overhauled. Gland packing renewed. Pressure test & leak test carried out prior fitting back. Valves found to be holding. All 3 valves fitted back. System tested, winches tried out. No leakages noticed","2021-07-02",null,"Completed","2021-05-24","No",null,null,"Internal"]
[null,null,null,null,null,"49_06/06/2021 4:16:16 PM","2021-05-23","Critical Equipment","Ship Staff","Ship Staff Insp.","Emergency generator output voltage found low, around 380V","LSA / FFA","Emgcy. Systems","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","troubleshooting carried out, found AVR defective, same replaced with new spare. Emgy genrator tried out found developing correct voltage 440V","2021-05-24",null,"Completed","2021-05-23","No",null,null,"Internal"]
[null,null,null,null,null,"49_06/06/2021 4:22:43 PM","2021-06-04","Critical Equipment","Ship Staff","Ship Staff Insp.","Stbd Lifeboat engine found not starting","Critical Equip.,LSA / FFA","Safety / LSA / FFA","Equipment Related",5.29,"High","Not Applicable","Not Applicable","Troubleshooting carried out, found one fuel pump stuck, same replaced with new pump. Sump oil replenish 2-3 times. Engine tried out found working satisfactory","2021-06-04",null,"Completed","2021-06-04","No",null,null,"Internal"]

{"sheet":"Calc","index":2,"n_rows":28,"n_cols":12,"rows_kept":28,"cut":false,"hidden":true,"merged":[]}
["Def_type","Def_cause","Equipments","VIQrefno","Observer_code"]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,"Dim itemSele As Long"]
[null,null,null,null,null,null,null,null,null,null,null,"   dim startRow as integer"]
[null,null,null,null,null,null,null,null,null,null,null,"   startRow=1"]
[null,null,null,null,null,null,null,null,null,null,null,"        For itemSele = 0 To ListBox1.ListCount - 1"]
[null,null,null,null,null,null,null,null,null,null,null,"        If ListBox1.Selected(itemSele) = True Then"]
[null,null,null,null,null,null,null,null,null,null,null,"        Worksheets(\"WorksheetName\").Range(\"A\" & startRow).Value = ListBox1.List(itemSele)"]
[null,null,null,null,null,null,null,null,null,null,null,"        startRow = startRow + 1"]
[null,null,null,null,null,null,null,null,null,null,null,"        End If"]
[null,null,null,null,null,null,null,null,null,null,null,"        Next"]
[null,null,null,null,null,null,null,null,null,null,null,"Dim LastRowA As String"]
[null,null,null,null,null,null,null,null,null,null,null,"        Dim itemSele As Long"]
[null,null,null,null,null,null,null,null,null,null,null,"       Dim startRow as integer"]
[null,null,null,null,null,null,null,null,null,null,null,"        LastRowA = ActiveSheet.Cells(Rows.count, \"A\").End(xlUp).row"]
[null,null,null,null,null,null,null,null,null,null,null,"        startQue = 0"]
[null,null,null,null,null,null,null,null,null,null,null,"        For itemSele = 0 To ListBox1.ListCount - 1"]
[null,null,null,null,null,null,null,null,null,null,null,"        For startRow = 1 To LastRowA"]
[null,null,null,null,null,null,null,null,null,null,null,"        If Worksheets(\"WorksheetName\").Range(\"A\" & startRow).Value = ListBox1.List(itemSele) Then"]
[null,null,null,null,null,null,null,null,null,null,null,"        ListBox1.Selected(itemSele) = True"]
[null,null,null,null,null,null,null,null,null,null,null,"        Exit For"]
[null,null,null,null,null,null,null,null,null,null,null,"        End If"]
[null,null,null,null,null,null,null,null,null,null,null,"        Next j"]
[null,null,null,null,null,null,null,null,null,null,null,"        Next"]
[null,null,null,null,null,null,null,null,null,null,null,"        End If"]

{"sheet":"Areaofobs","index":3,"n_rows":17,"n_cols":2,"rows_kept":17,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Cargo / Ballast Systems",11]
["Cert. & Docu.",2]
["Communication",6]
["Crew Management",3]
["Emgcy. Systems",13]
["Eng. / Strg. Comp.",14]
["General Appearance",15]
["Ice Opns.",17]
["ISM Related",7]
["ISPS Related",10]
["MARPOL Related",9]
["MLC Related",4]
["Mooring",12]
["Navigation",5]
["Safety / LSA / FFA",8]
["Structural Condn. / WT integrity ",16]

{"sheet":"Vessel_type","index":4,"n_rows":1,"n_cols":2,"rows_kept":1,"cut":false,"hidden":true,"merged":[]}
["Vessel_type","ID"]

{"sheet":"Deficiency_type","index":5,"n_rows":8,"n_cols":3,"rows_kept":8,"cut":false,"hidden":true,"merged":[]}
["TITLE","Type of deficiency_description","ID"]
["Breakdown",null,6]
["Critical Equipment",null,4]
["Defect",null,1]
["Guarantee Claim",null,8]
["Non Conformity",null,2]
["Observation",null,3]
["Other",null,7]

{"sheet":"VIQrefno","index":6,"n_rows":427,"n_cols":3,"rows_kept":427,"cut":false,"hidden":true,"merged":[]}
["VIQ_ref_no","Risk Value of observation","ID"]
["1.1","Low",8243]
["1.10","Low",8252]
["1.11","Low",8253]
["1.12","Low",8254]
["1.13","Low",8255]
["1.14","Low",8256]
["1.15","Low",8257]
["1.16","Low",8259]
["1.17","Low",8260]
["1.18","Low",8261]
["1.19","Low",8262]
["1.2","Low",8244]
["1.20","Low",8263]
["1.21","Low",8265]
["1.22","Low",8266]
["1.23","Low",8267]
["1.24","Low",8268]
["1.25","Low",8269]
["1.26","Low",8270]
["1.3","Low",8245]
["1.4","Low",8246]
["1.5","Low",8247]
["1.6","Low",8248]
["1.7","Low",8249]
["1.8","Low",8250]
["1.9","Low",8251]
["1.99","High",11258]
["10.1","Medium",8461]
["10.10","High",8470]
["10.11","Medium",8471]
["10.12","Very High",8472]
["10.13","Very High",8473]
["10.14","Medium",8474]
["10.15","Low",8475]
["10.16","Very High",8476]
["10.17","Very High",8477]
["10.18","High",8478]
["10.19","Very High",8479]
["10.2","Low",8462]
["10.20","High",8480]
["10.21","Medium",8481]
["10.22","Low",8482]
["10.23","Medium",8483]
["10.24","Low",8484]
["10.25","Very High",8485]
["10.26","High",8486]
["10.27","Medium",8487]
["10.28","Low",8488]
["10.29","Medium",8489]
["10.3","Medium",8463]
["10.30","High",8490]
["10.31","Very High",8491]
["10.32","Very High",8492]
["10.33","High",8493]
["10.34","High",8494]
["10.35","Very High",8495]
["10.36","Very High",8496]
["10.37","Medium",8497]
["10.38","Medium",8498]
["10.39","High",8499]
["10.4","High",8464]
["10.40","Medium",8500]
["10.41","Medium",8501]
["10.42","Medium",8502]
["10.43","Medium",8503]
["10.44","Medium",8504]
["10.45","Very High",8505]
["10.46","High",8506]
["10.47","Medium",8507]
["10.48","High",8508]
["10.49","Medium",8509]
["10.5","Low",8465]
["10.50","High",8510]
["10.51","Low",8511]
["10.52","Medium",8512]
["10.53","Medium",8513]
["10.54","High",8514]
["10.55","Low",8515]
["10.6","Very High",8466]
["10.7","Medium",8467]
["10.8","Medium",8468]
["10.9","Medium",8469]
["10.99","High",8516]
["11.1","High",8420]
["11.10","Medium",8429]
["11.11","Very High",8430]
["11.12","Low",8431]
["11.13","Low",8432]
["11.14","Medium",8433]
["11.15","Low",8434]
["11.16","Low",8435]
["11.17","Low",8436]
["11.2","Medium",8421]
["11.3","Medium",8422]
["11.4","Very High",8423]
["11.5","Medium",8424]
["11.6","Medium",8425]
["11.7","High",8426]
["11.8","Low",8427]
["11.9","Low",8428]
["11.99","High",8437]
["12.1","High",8438]
["12.10","High",8448]
["12.11","High",8449]
["12.12","High",8450]
["12.13","High",8451]
["12.14","High",8452]
["12.15","High",8453]
["12.16","High",8454]
["12.17","High",8455]
["12.18","High",8456]
["12.19","High",8457]
["12.2","High",8439]
["12.20","High",8458]
["12.21","High",8459]
["12.3","High",8441]
["12.4","High",8442]
["12.5","High",8443]
["12.6","High",8444]
["12.7","High",8445]
["12.8","High",8446]
["12.9","High",8447]
["12.99","High",8460]
["2.1","Very High",8296]
["2.1.9","Very High",11259]
["2.10","Medium",8304]
["2.11","Medium",8305]
["2.12","Low",8306]
["2.13","Low",8307]
["2.14","Low",8308]
["2.15","Low",8309]
["2.16","Medium",8310]
["2.2","Medium",8297]
["2.3","High",8295]
["2.4","Medium",8298]
["2.5","Medium",8299]
["2.6","Low",8300]
["2.7","High",8301]
["2.8","High",8302]
["2.9","Medium",8303]
["2.99","High",8311]
["3.1","High",8312]
["3.2","Very High",8313]
["3.3","High",8314]
["3.4","Low",8294]
["3.5","Medium",8315]
["3.6","High",8316]
["3.7","Very High",8317]
["3.8","Very High",8318]
["3.99","High",8319]
["4.1","High",8320]
["4.10","High",8329]
["4.11","Medium",8330]
["4.12","Very High",8331]
["4.13","Very High",8332]
["4.14","Very High",8333]
["4.15","Very High",8334]
["4.16","Very High",8335]
["4.17","Very High",8336]
["4.18","Very High",8337]
["4.19","Low",8338]
["4.2","Medium",8321]
["4.20","Very High",8339]
["4.21","High",8340]
["4.22","Low",8341]
["4.23","High",8342]
["4.24","High",8343]
["4.25","Low",8344]
["4.26","Low",8345]
["4.27","High",8346]
["4.3","Medium",8322]
["4.4","High",8323]
["4.5","Very High",8324]
["4.6","Medium",8325]
["4.7","High",8326]
["4.8","Medium",8327]
["4.9","Medium",8328]
["4.99","High",8347]
["5.1","Very High",8517]
["5.10","High",8526]
["5.11","Low",8527]
["5.12","Medium",8528]
["5.13","High",8529]
["5.14","Very High",8530]
["5.15","Medium",8531]
["5.16","Very High",8532]
["5.17","Very High",8533]
["5.18","High",8534]
["5.19","Medium",8535]
["5.2","Very High",8518]
["5.20","Medium",8536]
["5.21","Medium",8537]
["5.22","High",8539]
["5.23","Very High",8540]
["5.24","Very High",8541]
["5.25","Medium",8542]
["5.26","Medium",8543]
["5.27","Medium",8544]
["5.28","Very High",8545]
["5.29","High",8546]
["5.3","Low",8519]
["5.30","High",8547]
["5.31","High",8548]
["5.32","High",8549]
["5.33","High",8550]
["5.34","Low",8551]
["5.35","Medium",8552]
["5.36","Low",8553]
["5.37","Low",8554]
["5.38","High",8555]
["5.39","Very High",8556]
["5.4","High",8520]
["5.40","Very High",8557]
["5.41","Very High",8558]
["5.42","Medium",8559]
["5.43","High",8560]
["5.44","High",8561]
["5.45","Medium",8564]
["5.46","Medium",8565]
["5.47","Medium",8566]
["5.48","Medium",8567]
["5.5","Low",8521]
["5.6","Low",8522]
["5.7","Medium",8523]
["5.8","Medium",8524]
["5.9","Very High",8525]
["5.99","High",8568]
["6.1","Medium",8348]
["6.10","Low",8357]
["6.11","High",8358]
["6.12","Medium",8359]
["6.13","Low",8360]
["6.14","High",8361]
["6.15","High",8362]
["6.16","Very High",8363]
["6.17","Very High",8364]
["6.18","Medium",8365]
["6.19","Low",8366]
["6.2","High",8349]
["6.20","Medium",8367]
["6.21","High",8368]
["6.22","Medium",8369]
["6.3","Low",8350]
["6.4","High",8351]
["6.5","Medium",8352]
["6.6","Medium",8353]
["6.7","High",8354]
["6.8","High",8355]
["6.9","Low",8356]
["6.99","High",8370]
["7.1","High",8371]
["7.10","High",8380]
["7.11","High",8381]
["7.12","High",8382]
["7.13","Medium",8383]
["7.14","Medium",8384]
["7.15","High",8385]
["7.16","High",8386]
["7.17","High",8387]
["7.2","High",8372]
["7.3","Low",8373]
["7.4","Low",8374]
["7.5","Low",8375]
["7.6","Medium",8376]
["7.7","Low",8377]
["7.8","High",8378]
["7.9","High",8379]
["7.99","High",8388]
["8.1","Very High",8569]
["8.10","Very High",8578]
["8.100","Low",11227]
["8.101","Medium",11228]
["8.102","Low",11229]
["8.103","Low",11230]
["8.104","Low",11231]
["8.105","Medium",11232]
["8.106","Medium",11233]
["8.107","Low",11234]
["8.108","High",11235]
["8.109","Very High",11236]
["8.11","Medium",8579]
["8.110","High",11237]
["8.111","Medium",11238]
["8.112","High",11239]
["8.113","Medium",11240]
["8.114","Low",11241]
["8.115","High",11242]
["8.116","Medium",11243]
["8.117","Medium",11244]
["8.118","Medium",11245]
["8.119","High",11246]
["8.12","Medium",8580]
["8.120","High",11247]
["8.121","Medium",11248]
["8.122","High",11249]
["8.123","High",11250]
["8.124","Low",11251]
["8.125","High",11252]
["8.126","Medium",11253]
["8.127","Medium",11254]
["8.13","Medium",8581]
["8.14","Very High",8582]
["8.15","High",8583]
["8.16","Very High",8584]
["8.17","Low",8585]
["8.18","High",8586]
["8.19","High",8587]
["8.199","High",11255]
["8.2","Medium",8570]
["8.20","Medium",8588]
["8.21","High",8589]
["8.22","Very High",8590]
["8.23","Medium",8591]
["8.24","Medium",8592]
["8.25","Very High",8593]
["8.26","High",8594]
["8.27","Medium",8595]
["8.28","Medium",8596]
["8.29","High",8598]
["8.3","Very High",8571]
["8.30","High",8599]
["8.31","High",8600]
["8.32","Low",8601]
["8.33","Medium",8602]
["8.34","High",8603]
["8.35","Medium",8604]
["8.36","Medium",8605]
["8.37","High",8607]
["8.38","Medium",8608]
["8.39","Medium",8609]
["8.4","Medium",8572]
["8.40","High",8610]
["8.41","Medium",8611]
["8.42","Medium",8612]
["8.43","Very High",8613]
["8.44","High",8615]
["8.45","High",8616]
["8.46","Very High",8617]
["8.47","Very High",8618]
["8.48","Medium",8619]
["8.49","High",8620]
["8.5","Very High",8573]
["8.50","Medium",8621]
["8.51","Low",8622]
["8.52","Low",8623]
["8.53","Low",8624]
["8.54","High",8625]
["8.55","Low",11182]
["8.56","Medium",11183]
["8.57","Medium",11184]
["8.58","High",11185]
["8.59","High",11186]
["8.6","Medium",8574]
["8.60","High",11187]
["8.61","Medium",11188]
["8.62","Very High",11189]
["8.63","High",11190]
["8.64","Medium",11191]
["8.65","Low",11192]
["8.66","High",11193]
["8.67","High",11194]
["8.68","High",11195]
["8.69","Medium",11196]
["8.7","High",8575]
["8.70","Medium",11197]
["8.71","Very High",11198]
["8.72","Medium",11199]
["8.73","Medium",11200]
["8.74","High",11201]
["8.75","Medium",11202]
["8.76","Medium",11203]
["8.77","Medium",11204]
["8.78","Medium",11205]
["8.79","Medium",11206]
["8.8","Medium",8576]
["8.80","Medium",11207]
["8.81","Low",11208]
["8.82","Medium",11209]
["8.83","Low",11210]
["8.84","Low",11211]
["8.85","Medium",11212]
["8.86","Medium",11213]
["8.87","Medium",11214]
["8.88","Low",11215]
["8.89","High",11216]
["8.9","High",8577]
["8.90","High",11217]
["8.91","High",11218]
["8.92","Medium",11219]
["8.93","Low",11220]
["8.94","Low",11221]
["8.95","Medium",11222]
["8.96","Medium",11223]
["8.97","Low",11224]
["8.98","High",11225]
["8.99","Medium",11226]
["9.1","Low",8390]
["9.10","Medium",8399]
["9.11","Medium",8400]
["9.12","Medium",8401]
["9.13","Low",8402]
["9.14","Medium",8403]
["9.15","Medium",8404]
["9.16","High",8405]
["9.17","High",8406]
["9.18","Low",8407]
["9.19","Low",8408]
["9.2","Very High",8391]
["9.20","Medium",8409]
["9.21","Medium",8410]
["9.22","Low",8411]
["9.23","Low",8412]
["9.24","Medium",8413]
["9.25","Low",8414]
["9.26","Low",8415]
["9.27","Low",8416]
["9.28","Medium",8417]
["9.29","Low",8418]
["9.3","Very High",8392]
["9.4","High",8393]
["9.5","High",8394]
["9.6","Low",8395]
["9.7","Medium",8396]
["9.8","Medium",8397]
["9.9","Medium",8398]
["9.99","High",8419]

{"sheet":"Equipment_list","index":7,"n_rows":28,"n_cols":3,"rows_kept":28,"cut":false,"hidden":true,"merged":[]}
["TITLE","Equipment_list_description","ID"]
["Accommodation",null,12]
["Cargo Mach.",null,13]
["Critical Equip.",null,16]
["Deck - Machinery",null,18]
["Deck - Mooring Machinery",null,15]
["Deck - Pipe / Fittings",null,20]
["Documentation",null,21]
["E/R - Air Comp.",null,8]
["E/R - Aux. Engine",null,4]
["E/R - Aux. Mach.",null,7]
["E/R - Boiler",null,5]
["E/R - Main Engine",null,3]
["E/R - Pipes/ valves & fittings",null,9]
["E/R - Pumps",null,32]
["E/R - Purifier",null,6]
["Elect. Mach. & Equip.",null,10]
["Hull & Tanks",null,19]
["Inert Gas",null,14]
["LSA / FFA",null,17]
["Miscellaneous",null,22]
["Navigation - DGPS / EPFS / AIS",null,28]
["Navigation - ECDIS",null,25]
["Navigation - Echo Sounder / Speed Log",null,26]
["Navigation - GMDSS & Communication",null,23]
["Navigation - Others",null,11]
["Navigation - RADAR",null,24]
["Navigation - VDR / BNWAS",null,30]

{"sheet":"PSC_MOU","index":8,"n_rows":11,"n_cols":3,"rows_kept":11,"cut":false,"hidden":true,"merged":[]}
["TITLE","PSC_MOU_description","ID"]
["Asia and the Pacific",null,2]
["Caribbean",null,4]
["Europe and the North Atlantic",null,1]
["Latin America",null,3]
["The Black Sea region",null,6]
["The Indian Ocean",null,8]
["The Mediterranean",null,7]
["The Riyadh MoU",null,9]
["USCG",null,10]
["West and Central Africa",null,5]

{"sheet":"Inspection_type","index":9,"n_rows":13,"n_cols":2,"rows_kept":13,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Bunkering Audit",14]
["Cargo Audit",17]
["Engineering Audit",16]
["ISM Audit",2]
["ISPS Audit",3]
["IT Audit",10]
["MLC Audit",1]
["Mooring Audit",9]
["Nav Audit / Verification",8]
["Onboard Training",18]
["Ship Staff Insp.",15]
["Suptd. Insp.",13]

{"sheet":"Deficiency_Cause","index":10,"n_rows":8,"n_cols":3,"rows_kept":8,"cut":false,"hidden":true,"merged":[]}
["TITLE","Deficiency_Cause_description","ID"]
["Behaviour Based",null,1]
["Equipment Related",null,4]
["External Factors",null,5]
["Human Error",null,7]
["Inappropriate Procedure",null,8]
["Industry Issue",null,6]
["Knowledge Based",null,3]

{"sheet":"Observer_code","index":11,"n_rows":3,"n_cols":3,"rows_kept":3,"cut":false,"hidden":true,"merged":[]}
["TITLE","Observer_code_description","ID"]
["Owner / Marine / Tech. Suptd.",null,3]
["Ship Staff",null,2]

{"sheet":"Status_code","index":12,"n_rows":6,"n_cols":3,"rows_kept":6,"cut":false,"hidden":true,"merged":[]}
["TITLE","Status_code_description","ID"]
["Completed",null,6]
["Deferred to D D",null,5]
["In progress",null,3]
["Not Started",null,2]
["Waiting spare",null,4]

{"sheet":"PSC_ref_no","index":13,"n_rows":19,"n_cols":2,"rows_kept":19,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Alarms",9]
["Cargo operations including equipment",7]
["Certificates & Documentation",2]
["Dangerous Goods",13]
["Emergency Systems",5]
["Fire safety",8]
["ISM",16]
["ISPS",17]
["Life saving appliances",12]
["MLC, 2006",18]
["Other",19]
["Pollution Prevention",15]
["Propulsion and auxiliary machinery",14]
["Radio communication",6]
["Safety of Navigation",11]
["Structural condition",3]
["Water/Weathertight condition",4]
["Working and Living Conditions",10]

{"sheet":"Risk_value_of_obs","index":14,"n_rows":1,"n_cols":2,"rows_kept":1,"cut":false,"hidden":true,"merged":[]}
["Risk Value of observation","ID"]

{"sheet":"Year","index":15,"n_rows":18,"n_cols":1,"rows_kept":18,"cut":false,"hidden":true,"merged":[]}
["Year"]
[2014]
[2015]
[2016]
[2017]
[2018]
[2019]
[2020]
[2021]
[2022]
[2023]
[2024]
[2025]
[2026]
[2027]
[2028]
[2029]
[2030]

{"sheet":"Month","index":16,"n_rows":13,"n_cols":1,"rows_kept":13,"cut":false,"hidden":true,"merged":[]}
["Month"]
["Jan"]
["Feb"]
["Mar"]
["Apr"]
["May"]
["Jun"]
["Jul"]
["Aug"]
["Sep"]
["Oct"]
["Nov"]
["Dec"]

{"sheet":"Date_","index":17,"n_rows":32,"n_cols":1,"rows_kept":32,"cut":false,"hidden":true,"merged":[]}
["Date"]
["01"]
["02"]
["03"]
["04"]
["05"]
["06"]
["07"]
["08"]
["09"]
[10]
[11]
[12]
[13]
[14]
[15]
[16]
[17]
[18]
[19]
[20]
[21]
[22]
[23]
[24]
[25]
[26]
[27]
[28]
[29]
[30]
[31]

{"sheet":"Sheet1","index":18,"n_rows":24,"n_cols":6,"rows_kept":24,"cut":false,"hidden":true,"merged":[]}
[]
[null,"ID","E",null,"Date Recorded",1]
[null,"UNIQUE ID","F",null,"Type of Deficiency",2]
[1,"Date Recorded","G",null,"Observer code",3]
["ignore","Vessel Type","H",null,"Type of Inspection",4]
[null,"Internal / External","I",null,"Description of Deficiency",5]
[null,"Drydock","J",null,"Equipment Categories",6]
[null,"Information Sharing","K",null,"Area of Observation",7]
[null,"Critical_item","L",null,"Deficiency Cause",8]
[null,"Deficiency Type","M",null,"VIQ Ref Number",9]
[null,"Deficiency Cause","N",null,"Risk Value of Obs",10]
[null,"Inspection Type","O",null,"PSC Ref Number",11]
[null,"Equipments","P",null,"PSC MOU ID",12]
[null,"VIQ Reference Number","Q",null,"Action Taken or Required",13]
[null,"Risk Value of the observation","R",null,"Target Date",14]
[null,"PSC Reference Number","S",null,"PO Ref No.",15]
[null,"PSC MOU","T",null,"Status Code",16]
[null,"Observer Code","U",null,"Date Completed",17]
[null,"Target Date","V",null,"Drydock",18]
[null,"Status Code","W",null,"Info Sharing",19]
[null,"Description of Deficiency","X",null,"Critical Item Flag",20]
[null,"Action taken / required","Y",null,"Audit Type",21]
[null,"PO ref no","Z"]
[null,"Date completed","AA"]

{"sheet":"Ship_information","index":19,"n_rows":2,"n_cols":3,"rows_kept":2,"cut":false,"hidden":true,"merged":[]}
["Ship_ID","Ship_Name","FILE_NAME"]
["49","RESPECT (29-04-2021)","49_1622271684231.xlsm"]

{"sheet":"External_Deficiency_type","index":20,"n_rows":5,"n_cols":3,"rows_kept":5,"cut":false,"hidden":true,"merged":[]}
["TITLE","Type of deficiency_description","ID"]
["Condn of Class / Memo",null,5]
["Defect",null,1]
["Non Conformity",null,2]
["Observation",null,3]

{"sheet":"External_Inspection_type","index":21,"n_rows":11,"n_cols":2,"rows_kept":11,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Cargo Audit",17]
["Flag State Insp.",5]
["ISM Audit",2]
["ISPS Audit",3]
["MLC Audit",1]
["Nav Audit / Verification",8]
["OM Insp. (Eg. SIRE / CDI etc.)",6]
["Others (Eg. Insurance etc.)",12]
["PSC Inspection",4]
["Terminal Insp.",11]

{"sheet":"External_Observer_code","index":22,"n_rows":7,"n_cols":3,"rows_kept":7,"cut":false,"hidden":true,"merged":[]}
["TITLE","Observer_code_description","ID"]
["Class Surveyor",null,4]
["FSC Inspector",null,5]
["Others (Eg. Insurance etc.)",null,9]
["PSC Insp.",null,6]
["SIRE / CDI Insp.",null,8]
["Terminal Insp.",null,7]

{"sheet":"Sheet Version","index":23,"n_rows":2,"n_cols":2,"rows_kept":2,"cut":false,"hidden":true,"merged":[]}
["Version","Title"]
["2.0","Version 2.0"]