{"text_format":"1","workbook":"xlsx","n_sheets":24,"sheets":["Mainsheet","Completed","Calc","Areaofobs","Vessel_type","Deficiency_type","VIQrefno","Equipment_list","PSC_MOU","Inspection_type","Deficiency_Cause","Observer_code","Status_code","PSC_ref_no","Risk_value_of_obs","Year","Month","Date_","Sheet1","Ship_information","External_Deficiency_type","External_Inspection_type","External_Observer_code","Sheet Version"],"not_rendered":{"charts":0,"images":5,"macros":1,"external_links":0,"defined_names":12,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Mainsheet","index":0,"n_rows":28,"n_cols":28,"rows_kept":28,"cut":false,"hidden":false,"merged":[[10,8,10,9],[10,12,10,13],[12,6,12,27],[8,6,8,27]]}
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,"Defect - Damage Monitoring Sheet"]
[]
[null,null,null,null,null,null,null,"Date of Report","2021-06-16",null,null,"Ship Name","WAWASAN RUBY (05-06-2021)"]
[]
[null,null,null,null,null,null,"VERSION : 2.0"]
[]
[]
[]
[null,null,null,null,"ID","UNIQUE ID","Date Recorded","Type of Deficiency","Observer code","Type of Inspection","Description of Deficiency","Equipment Categories","Area of Observation","Deficiency Cause","VIQ Ref Number","Risk Value of Obs","PSC Ref Number","PSC MOU ID","Action Taken or Required","Target Date","PO Ref No.","Status Code","Date Completed","Drydock","Info Sharing","Critical Item","Audit Type","Superintendent Remarks"]
[null,null,null,null,18173,"46_31-Jan-21 4:03:06 PM","2021-01-18","Defect","Ship Staff","Ship Staff Insp.","The tank cleaning heater water level gauge  found defective and glass broken.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related",8.18,"Low","Not Applicable","Not Applicable","Level Gauge glass tube size (L = 450 mm, D = 13 mm, T = 2 mm). Vsl. will send a requisition for supplying a required spare on arrival Singapore","2021-06-30","WRUB210139","Waiting spare",null,"No","No","No","Internal","PLEASE ADVICE IF ALTERNATIVE ARRANGEMENT IS DONE FOR THIS AT PRESENT. ALSO TO SEND US DIMENSIONS OF GLASS TUBE (LENGTH, HEIGHT,DIAMETER, THICKNESS) WHICH COULD BE PROCURED EASILY IN INDIAN PORTS."]
[null,null,null,null,18783,"46_26/03/2021 9:52:06 PM","2021-03-24","Observation","Owner / Marine / Tech. Suptd.","ISM Audit","Mooring ropes 5 nos are not in good condition and the present certs onboard the MBL is higher than the SDMBL","Miscellaneous","Mooring","Equipment Related,Knowledge Based",9.5,"High","Not Applicable","Not Applicable","New Ropes rec'd on 15th May'21 at Singapore. Same will be fitted in place at the earliest","2021-06-23","WRUB210084","In progress",null,"No","No","No","Internal","NEW MOORING ROPES ALREADY PROCURED AND WILL BE CONNECTED ON BOARD DURING SINGAPORE CALL MAY 2021."]
[null,null,null,null,18779,"46_15/04/2021 12:34:50 PM","2021-04-06","Defect","Ship Staff","Ship Staff Insp.","9S cargo tank giving false High level alarm even though tank was empty.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related",8.23,"Medium","Not Applicable","Not Applicable","Investigation is in progress. Planning to complete  the rectification work soon after receiving the spare","2021-06-30","WRUB215018","Waiting spare",null,"No","No","No","Internal","SPARES ORDERED AND WILL BE READY BY 21ST MAY 2021. WE WILL CONNECT IMMEDAITELY. TILL THAT PERIOD ADDITIONAL MONITORING TO EXCERCISE."]
[null,null,null,null,18781,"46_15/03/2021 9:06:07 AM","2021-04-15","Defect","Ship Staff","Ship Staff Insp.","BOILER FUEL OIL SUPPLY PUMP DUPLEX FILTER CHANGE OVER MECHANISM NOT HOLDING","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","FILTER NEED TO BE REPLACED,REQUISITION RAISED FOR THE SAME","2021-06-30","WRUB210072","Waiting spare",null,"No","No","No","Internal","SPARES ORDERED AND WILL BE READY BY 15TH MAY. WE WILL CONNECT SPARES TO VESSEL ONCE READY.  ENSURE PRECAUTIONS ARE TAKEN FOR CHANGEOVER AND IT IS DONE WITH PUMP IN OFF CONDITION."]
[null,null,null,null,18177,"46_28/02/2021 3:56:10 PM","2021-04-28","Defect","Ship Staff","Ship Staff Insp.","Main Engine Lube oil Auto temperature controller not functional.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Requisition raised for controller cylinder ram unit. ","2021-06-30","WRUB210049","Waiting spare",null,"No","No","No","Internal","PLEASE PROVIDE TECHNICAL UPDATE ON THIS TO PROCEED FURTHER."]
[null,null,null,null,null,"46_16/06/2021 8:17:19 PM","2021-06-16","Defect","Ship Staff","Ship Staff Insp.","Main engine shaft  power meter defective","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Shaft power meter calibration need to be carried out. OFFICE TO ARRANGE TECHNICIAN","2021-07-31","WRUB210140","Not Started",null,"No",null,null,"Internal"]
[null,null,null,null,null,"46_16/06/2021 8:31:01 PM","2021-06-16","Defect","Ship Staff","Ship Staff Insp.","Fire and G/S pump Discharge v/v is not holding","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Requision raised","2021-07-31","WRUB210139","Waiting spare",null,"No",null,null,"Internal"]
[null,null,null,null,null,"46_16/06/2021 8:39:49 PM","2021-06-16","Defect","Ship Staff","Ship Staff Insp.","waste oil tank level gauge defective ","Miscellaneous","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Requistion raised. ","2021-07-31","WRUB210139","Waiting spare",null,"No",null,null,"Internal"]
[null,null,null,null,null,"46_16/06/2021 8:44:42 PM","2021-06-16","Defect","Ship Staff","Ship Staff Insp.","Main air compressor no 1 NRV defective ","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Requistion WRUB 215031 raised and waiting for spares","2021-07-31","WRUB 215031","Waiting spare",null,"No",null,null,"Internal"]
[null,null,null,null,null,"46_16/06/2021 8:34:26 PM","2021-06-16","Defect","Ship Staff","Ship Staff Insp.","Bunker line FO stbd tk inlet v/v not holding ","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Requistion  raised. ","2021-07-31","WRUB210139","Waiting spare",null,"No",null,null,"Internal"]
[null,null,null,null,null,"46_18/06/2021 10:09:02 AM","2021-06-17","Defect","Ship Staff","Ship Staff Insp.","SEWAGE TANK OUTLET VALVE DEFECTIVE","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","REQUISITION MADE","2021-07-31","WRUB210139","Waiting spare",null,"No",null,null,"Internal"]

{"sheet":"Completed","index":1,"n_rows":452,"n_cols":28,"rows_kept":452,"cut":false,"hidden":false,"merged":[[10,8,10,9],[10,12,10,13],[12,6,12,27],[8,6,8,27]]}
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,"Defect - Damage Monitoring Sheet"]
[]
[null,null,null,null,null,null,null,"Date of Report","29-Apr-2021",null,null,"Ship Name","WAWASAN RUBY (29-04-2021)"]
[]
[null,null,null,null,null,null,"VERSION : 2.0"]
[]
[]
[]
[null,null,null,null,"ID","UNIQUE ID","Date Recorded","Type of Deficiency","Observer code","Type of Inspection","Description of Deficiency","Equipment Categories","Area of Observation","Deficiency Cause","VIQ Ref Number","Risk Value of Obs","PSC Ref Number","PSC MOU ID","Action Taken or Required","Target Date","PO Ref No.","Status Code","Date Completed","Drydock","Info Sharing","Critical Item","Audit Type","Superintendent Remarks"]
[null,null,null,null,5455,"46_2019-10-24 09:30:09.000","2019-01-01","Defect","Ship Staff","Ship Staff Insp.","AUX CONDENSOR SW OUTLET  LEAKAGE","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","LEAK RECTIFIED","2019-01-31","","Completed","2019-01-26","No","No","No","Internal"]
[null,null,null,null,5470,"46_2019-10-24 11:12:29.000","2019-01-01","Defect","Ship Staff","Ship Staff Insp.","AUX SW PUMP SUCTION VALVE LEAKS","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Suction valve overhauled","2019-03-31","","Completed","2019-03-16","No","No","No","Internal"]
[null,null,null,null,5451,"46_2019-10-23 10:42:28.999","2019-01-07","Defect","Ship Staff","Ship Staff Insp.","2 tank cleaning machine not working","Deck - Machinery","Cargo / Ballast Systems","Equipment Related","8.29","Medium","","","tank cleaning machine overhauled. working normal","2019-01-08","WRUB180309","Completed","2019-01-14","No","No","No","Internal"]
[null,null,null,null,5452,"46_2019-10-23 10:47:58.999","2019-01-08","Defect","Ship Staff","Ship Staff Insp.","Telegraph indication light not working ","Navigation - Others","Navigation","Equipment Related","4.7","High","","","light changed. tested working normal","2019-01-13","","Completed","2019-01-13","No","No","No","Internal"]
[null,null,null,null,5454,"46_2019-10-24 09:23:50.000","2019-01-12","Defect","Ship Staff","Ship Staff Insp.","ER STORE HAS VERY POOR VENTILLATION AND LIGHTING","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","external fan installed in E/R store and number of lights increased.","2019-01-31","","Completed","2019-01-24","No","No","No","Internal"]
[null,null,null,null,5481,"46_25/10/2019 6:58:35 AM","2019-01-14","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp."," Arrange provision stores.","Miscellaneous","General Appearance","Behaviour Based,Human Error,Inappropriate Procedure","11.12","Low","","","provision store arranged","2019-01-25","","Completed","2019-01-20","No","No","No","Internal"]
[null,null,null,null,5453,"46_2019-10-24 09:15:36.000","2019-01-15","Defect","Ship Staff","Ship Staff Insp.","6S manifold valve stbd side leaking","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.3","Medium","","","6S manifold valve stbd side overhauled.SS seat ring renewed","2019-01-31","","Completed","2019-01-17","No","No","No","Internal"]
[null,null,null,null,5472,"46_25/10/2019 5:54:40 AM","2019-01-17","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Gyro repeater glass frame to be cleaned.","Navigation - Others","Navigation","Behaviour Based,Human Error,Inappropriate Procedure","4.9","Medium","","","Gyro repeater glass frame cleaned.","2019-01-27","","Completed","2019-01-18","No","No","No","Internal"]
[null,null,null,null,5473,"46_25/10/2019 5:59:15 AM","2019-01-17","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","CO2 natural vent port upper deck not stencil.","Miscellaneous","General Appearance","Human Error","11.3","Medium","","","CO2 natural vent port upper deck stencilling carried out.","2019-01-24","","Completed","2019-01-18","No","No","No","Internal"]
[null,null,null,null,5474,"46_25/10/2019 6:02:13 AM","2019-01-17","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp."," High voltage sticker on mf/hf antenna to be renewed.","Miscellaneous","General Appearance","Human Error","11.3","Medium","",""," High voltage sticker on mf/hf antenna renewed.","2019-01-27","","Completed","2019-01-22","No","No","No","Internal"]
[null,null,null,null,5475,"46_25/10/2019 6:10:04 AM","2019-01-17","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Cleaning of accommodation vent wire mesh/filter to be done.","Miscellaneous","General Appearance","Inappropriate Procedure","11.7","High","","","Cleaning of accommodation vent wire mesh/filter carried out.","2019-01-27","","Completed","2019-01-20","No","No","No","Internal"]
[null,null,null,null,5476,"46_25/10/2019 6:14:40 AM","2019-01-17","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Life boats fwd. hatch buff and grease the hinge of fwd. hatch, buffing and painting of hatch handle to be done.","LSA / FFA","Safety / LSA / FFA","Human Error,Inappropriate Procedure","5.29","High","","","greasing, buffing and painting carried out","2019-01-30","","Completed","2019-01-24","No","No","No","Internal"]
[null,null,null,null,5477,"46_25/10/2019 6:07:08 AM","2019-01-17","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp."," Funnel cleaning and painting to be done.","Miscellaneous","General Appearance","Human Error,Inappropriate Procedure","11.8","Low","","","funnel area cleaned, derusted and painted","2019-01-31","","Completed","2019-01-29","No","No","No","Internal"]
[null,null,null,null,5478,"46_25/10/2019 6:22:40 AM","2019-01-17","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp."," Life boat launch instructions stbd side missing to be renewed/ stenciled.","LSA / FFA","Safety / LSA / FFA","Behaviour Based,Human Error,Inappropriate Procedure","5.3","Low","","","new instruction card posted","2019-01-27","","Completed","2019-01-21","No","No","No","Internal"]
[null,null,null,null,5479,"46_25/10/2019 6:25:48 AM","2019-01-17","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp."," Cargo hose markings to be renewed.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Inappropriate Procedure","8.8","Very High","","","cargo hose marking carried out","2019-01-27","","Completed","2019-01-24","No","No","No","Internal"]
[null,null,null,null,5480,"46_25/10/2019 6:54:53 AM","2019-01-17","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Fire door fire retardant packing to be renewed.","LSA / FFA","Safety / LSA / FFA","Human Error,Inappropriate Procedure","5.35","Medium","","","packing renewed","2019-01-30","","Completed","2019-01-22","No","No","No","Internal"]
[null,null,null,null,5482,"46_25/10/2019 6:31:00 AM","2019-01-17","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","  Mooring winch brake retaining nuts to be adjusted to 5mm.","Deck - Mooring Machinery","Mooring","Inappropriate Procedure","9.14","Medium","","","adjusted","2019-01-27","","Completed","2019-01-20","No","No","No","Internal"]
[null,null,null,null,5483,"46_25/10/2019 7:00:48 AM","2019-01-17","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Hospital flooring to be painted.","Miscellaneous","General Appearance","Human Error,Inappropriate Procedure","11.15","Low","","","hospital floor painted","2019-01-27","","Completed","2019-01-23","No","No","No","Internal"]
[null,null,null,null,5493,"46_2019-10-25 09:15:47.999","2019-01-17","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Whipping of MOB marker rope end to be done.","LSA / FFA","Safety / LSA / FFA","Inappropriate Procedure","5.31","High","","","WHIPPING DONE","2019-01-27","","Completed","2019-01-20","No","No","No","Internal"]
[null,null,null,null,5494,"46_2019-10-25 09:18:19.000","2019-01-17","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp."," Damaged tank dome rubber packing to be renewed.","Hull & Tanks","Cargo / Ballast Systems","Equipment Related","8.21","Medium","",""," Damaged tank dome rubber packing renewed.","2019-01-31","","Completed","2019-01-29","No","No","No","Internal"]
[null,null,null,null,5499,"46_2019-10-25 09:51:43.000","2019-01-17","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","  7S ballast tank manhole handle to be fabricated.","Hull & Tanks","Cargo / Ballast Systems","Equipment Related","11.3","Medium","","","handle fabricated","2019-01-30","","Completed","2019-01-27","No","No","No","Internal"]
[null,null,null,null,5501,"46_2019-10-25 10:02:16.000","2019-01-17","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp."," Mooring areas anti-skid paint to be applied.","Miscellaneous","Mooring","Inappropriate Procedure","9.13","Low","","","anti skid pain applied","2019-01-31","WRUB190103","Completed","2019-01-30","No","No","No","Internal"]
[null,null,null,null,5502,"46_2019-10-25 10:07:51.999","2019-01-17","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Stenciling of emergency framo connection point and yellow painting of emergency framo connection point to be done.","Deck - Pipe / Fittings","General Appearance","Inappropriate Procedure","11.3","Medium","","","stencilling completed","2019-01-27","","Completed","2019-01-22","No","No","No","Internal"]
[null,null,null,null,5533,"46_2019-10-26 09:21:33.000","2019-01-17","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Officer mess room music system not working.","Accommodation,Miscellaneous","MLC Related","Equipment Related","","","","","New music system received and placed","2019-01-31","WRUB190094","Completed","2019-01-21","No","No","No","Internal"]
[null,null,null,null,5463,"46_2019-10-24 10:40:54.000","2019-01-20","Defect","Ship Staff","Ship Staff Insp.","AUX ENG#3 LUB. OIL AUTO FILTER LEAKING FROM SHAFT MOTOR  SEAL","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Shaft motor replaced with spare received ","2019-10-30","WRUB190020","Completed","2019-10-24","No","No","No","Internal"]
[null,null,null,null,5456,"46_2019-10-24 09:36:16.000","2019-02-04","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Eye wash in steering chemical locker missing","Miscellaneous","","Behaviour Based,Human Error,Knowledge Based","5.46","Medium","","","New eye wash kept in steering gear first aid kit","2019-02-15","","Completed","2019-02-12","No","No","No","Internal"]
[null,null,null,null,5457,"46_2019-10-24 09:40:48.000","2019-02-04","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Port side L/R entrance globe bulb guard broken","LSA / FFA","Safety / LSA / FFA","Equipment Related","11.9","Low","","","new guard fitted","2019-02-18","","Completed","2019-02-08","No","No","No","Internal"]
[null,null,null,null,5458,"46_2019-10-24 09:44:13.999","2019-02-04","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","stbd side L/R entrance globe bulb unscrewed","LSA / FFA","Safety / LSA / FFA","Equipment Related,Human Error,Inappropriate Procedure","11.9","Low","","","screw fitted and tight","2019-02-18","","Completed","2019-02-08","No","No","No","Internal"]
[null,null,null,null,5459,"46_2019-10-24 09:47:26.999","2019-02-04","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Foam liquid pp,N2 fan & FW pp,no.1 steering panel source light fused ,all panel lights to recheck","LSA / FFA","Safety / LSA / FFA","Behaviour Based,Equipment Related,Human Error,Inappropriate Procedure","11.9","Low","","","all panel light checked and changed as required","2019-02-18","","Completed","2019-02-08","No","No","No","Internal"]
[null,null,null,null,5464,"46_2019-10-24 10:48:42.000","2019-02-04","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","IMO symbol for embarkation ladder broken, all IMO symbol on deck to be checked.","LSA / FFA","Safety / LSA / FFA","Behaviour Based,Inappropriate Procedure","5.47","Low","","","All IMO symbol checked and replaced as required","2019-02-18","","Completed","2019-02-25","No","No","No","Internal"]
[null,null,null,null,5465,"46_2019-10-24 10:52:46.000","2019-02-04","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","One of the Crew urinal was not in operation & covered. This MLC & PSC deficiency, rectify immediately.","Accommodation,Miscellaneous","MLC Related","Equipment Related,Human Error,Inappropriate Procedure","11.13","Low","","","Crew urinal cleaned and choke clear. working normal","2019-02-18","","Completed","2019-02-25","No","No","No","Internal"]
[null,null,null,null,5466,"46_2019-10-24 10:55:22.000","2019-02-04","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","6P, 5S, 5S, 2S gauge doesn’t have safety steel cover, either fabricate cover or change with original Framo & put the original cover","Deck - Pipe / Fittings","Cargo / Ballast Systems","Behaviour Based,Human Error,Inappropriate Procedure,Knowledge Based","8.13","Low","","","New steal cover fabricated and fixed in place","2019-02-28","","Completed","2019-02-25","No","No","No","Internal"]
[null,null,null,null,5467,"46_2019-10-24 10:59:13.000","2019-02-04","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Boiler Circulating Pump#2 Leaking","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Gland packing renewed","2019-03-15","","Completed","2019-02-26","No","No","No","Internal"]
[null,null,null,null,5469,"46_2019-10-24 11:09:12.000","2019-02-04","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Both side of windlass gear cover is broken, same to be removed, taken to WS & Rewelded.","Deck - Mooring Machinery","Mooring","Equipment Related","9.2","Very High","","","Windlass gear cover fabricated and same fitted in place","2019-02-28","","Completed","2019-03-04","No","No","No","Internal"]
[null,null,null,null,5471,"46_25/10/2019 5:51:23 AM","2019-02-04","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Trolley is not fabricated properly, same to be refabricated with large carrying capacity, the width should be slightly smaller of catwalk grating & should have handle.","Miscellaneous","General Appearance","Equipment Related","","","","","Trolley fabricated as require","2019-03-15","","Completed","2019-03-16","No","No","No","Internal"]
[null,null,null,null,5492,"46_25/10/2019 7:57:39 AM","2019-02-04","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Control Air Dryer Auto Drain Valve not working","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","same fitted in place tried out satisfactory","2019-04-10","","Completed","2019-04-07","No","No","No","Internal"]
[null,null,null,null,5460,"46_2019-10-24 09:56:39.000","2019-02-22","Defect","Ship Staff","Ship Staff Insp.","Deck fire & Foam line U clamp to be removed, rubber gaskets/Teflon sheets to be fitted beneath in order to avoid rusting of pipes from bottom.","Deck - Pipe / Fittings","Safety / LSA / FFA","Equipment Related","11.5","Medium","","","all U clamps removed and teflon sheet fitted to avoid rusting of pipes","2019-04-25","","Completed","2019-03-05","No","No","No","Internal"]
[null,null,null,null,5461,"46_2019-10-24 10:31:17.000","2019-02-24","Defect","Ship Staff","Ship Staff Insp.","1S, 8P & 8S Framo pressure gauge broken,","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.13","Low","","","Pressure gauge renewed with spare onboard","2019-02-28","","Completed","2019-02-26","No","No","No","Internal"]
[null,null,null,null,5462,"46_2019-10-24 10:35:02.999","2019-02-24","Defect","Ship Staff","Ship Staff Insp.","Deck steam drain near 10 S COT leaking from valve joint","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.15","Medium","","","Steam drain valve removed, cleaned and gasket renewd","2019-02-28","","Completed","2019-02-27","No","No","No","Internal"]
[null,null,null,null,5468,"46_2019-10-24 11:05:43.000","2019-02-26","Defect","Ship Staff","Ship Staff Insp.","ME Air Cooler Anode Flange Is Wasted and Leak ","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Gasket and anode renewed","2019-03-16","","Completed","2019-03-03","No","No","No","Internal"]
[null,null,null,null,5503,"46_2019-10-25 10:12:32.999","2019-02-26","Defect,Non Conformity","Ship Staff","Ship Staff Insp."," COT NO#3 (P) GAS PRESSURE AND TEMPERATURE  SENSOR SHOWING FAULTY READING","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.13","Low","","","Pressure sensor recevied and replaced , Mussasino technician inspected the system and installed 1K resistance however it was still showing faulty temp reading so mussasino technician's have asked to monitor the system and recommended to change radar and terminal board of 1P,2P,3P AND 4P COT","2019-05-30","WRUB190073","Completed","2019-04-18","No","No","No","Internal"]
[null,null,null,null,9747,"46_19/1/2020 4:24:13 AM","2019-03-04","Observation","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","Two spare lifejackets stowed in the safety equipment store, inside the\n\naccommodation on C deck starboard alley were found without any marking of ship's name and port of registry.","LSA / FFA","Safety / LSA / FFA","Behaviour Based,Human Error,Inappropriate Procedure","5.32","High","","","rectified imidiately","2019-03-08","","Completed","2019-03-04","No","No","No","External"]
[null,null,null,null,5490,"46_25/10/2019 7:38:52 AM","2019-03-04","Defect","Ship Staff","Ship Staff Insp.","Compressed Air Pipe Passing Thru Work Shop has several Pin Holes. This Pipe is not in Use but it is Common Line for Deck Air.Sign of SW ingress in the line caused Corrosion of Line .","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","job completed","2019-04-10","","Completed","2019-03-25","No","No","No","Internal"]
[null,null,null,null,5554,"46_26/10/2019 4:45:28 PM","2019-03-04","Defect","Ship Staff","Ship Staff Insp.","AE#3 Exhaust bellow is leaking after turbocharger.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","New bellow received and replaced iwth new one.","2019-08-30","WRUB190050","Completed","2019-10-04","No","No","No","Internal"]
[null,null,null,null,9666,"46_15/1/2020 8:50:24 PM","2019-03-04","Observation","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","the operators procedures in the mooring management plan sec -6 wear zone management stated frequency of rotating lines to different winches for wires only but did not include for mooring ropes.","Deck - Mooring Machinery","Mooring","Inappropriate Procedure","9.4","High","","","operators procedures was revised","2019-04-01","","Completed","2020-08-22","No","No","No","External"]
[null,null,null,null,5546,"46_26/10/2019 3:12:53 PM","2019-03-05","Defect","Ship Staff","Ship Staff Insp.","ECR A/C condenser end cover is corodded.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Cold repair work done before. Later spare was received and replaced with new one.","2019-06-05","WRUB 190079","Completed","2019-05-06","No","No","No","Internal"]
[null,null,null,null,5491,"46_25/10/2019 7:42:37 AM","2019-03-09","Defect","Ship Staff","Ship Staff Insp.","GLOBE STEAM VALVE  NO 7 AND  8 NOT HOLDING","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","11.4","Very High","","","lapping of steam valve carried out.","2019-04-15","","Completed","2019-04-06","No","No","No","Internal"]
[null,null,null,null,9582,"46_Mon Jan 13 2020 09:19:11 GMT+0000","2019-03-16","Observation","Owner / Marine / Tech. Suptd.","ISM Audit","Lifeboat lowering instructions ship specific not available under emergency light for Stbd lifeboat","LSA / FFA","Safety / LSA / FFA","Inappropriate Procedure","5.15","Medium","","","new poster made and pasted with a stronger adhesive.",null,"","Completed","2019-03-22","No","No","No","Internal"]
[null,null,null,null,9583,"46_Mon Jan 13 2020 09:31:47 GMT+0000","2019-03-16","Observation","Owner / Marine / Tech. Suptd.","ISM Audit","Fire doors 13 nos fire retardant packing require renewal","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.14","Very High","","","new packings installed on all the 13 doors.","2019-03-22","","Completed","2019-03-24","No","No","No","Internal"]
[null,null,null,null,9584,"46_Mon Jan 13 2020 09:36:32 GMT+0000","2019-03-16","Defect","Owner / Marine / Tech. Suptd.","ISM Audit","Deck airline in engine room holed at numerous places require renewal.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","New pipeline fabricated and fitted in place","2019-04-30","","Completed","2019-03-24","No","No","No","Internal"]
[null,null,null,null,9585,"46_Mon Jan 13 2020 09:39:44 GMT+0000","2019-03-16","Observation","Owner / Marine / Tech. Suptd.","ISM Audit","Aux Engines housekeeping to improve.","E/R - Aux. Engine","","Human Error","10.29","Medium","","","AUX engine area housekeeping improved by cleaning of aux engine machinery. spaces","2019-04-30","","Completed","2019-03-24","No","No","No","Internal"]
[null,null,null,null,9586,"46_Mon Jan 13 2020 09:42:16 GMT+0000","2019-03-16","Observation","Owner / Marine / Tech. Suptd.","MLC Audit","Hospital sanitary fittings, not clean fittings require maintenance/renewal","Accommodation","MLC Related","Human Error","11.15","Low","","","Fittings cleaned properly and renewed as required","2019-04-30","","Completed","2019-03-23","No","No","No","Internal"]
[null,null,null,null,9587,"46_Mon Jan 13 2020 09:44:57 GMT+0000","2019-03-16","Observation","Owner / Marine / Tech. Suptd.","MLC Audit","Galley utensils to be renewed as heavily carboned from the bottom","Accommodation","General Appearance","Equipment Related","11.13","Low","","","All the galley utensils checked for carbon deposits at the bottom. cleaned the same.","2019-04-30","","Completed","2019-03-22","No","No","No","Internal"]
[null,null,null,null,9588,"46_Mon Jan 13 2020 09:47:53 GMT+0000","2019-03-16","Observation","Owner / Marine / Tech. Suptd.","MLC Audit","Galley hot plate grill choked same to be cleaned","Accommodation","","Equipment Related","11.13","Low","","","grills of the hot plates were properly cleaned and all the holes were cleared.","2019-03-31","","Completed","2019-03-20","No","No","No","Internal"]
[null,null,null,null,9589,"46_Mon Jan 13 2020 09:50:10 GMT+0000","2019-03-16","Observation","Owner / Marine / Tech. Suptd.","Cargo Audit","Manual comparison between Remote/Local for Pressure not carried out witnessed only for Ullage and Temperature","Documentation","Cargo / Ballast Systems","Inappropriate Procedure","8.26","Low","","","started recording the ullage, pressure, and temperature comparison in the port log.","2019-04-30","","Completed","2019-03-20","No","No","No","Internal"]
[null,null,null,null,9590,"46_Mon Jan 13 2020 09:56:48 GMT+0000","2019-03-16","Observation","Owner / Marine / Tech. Suptd.","Cargo Audit","Working on pressure vessels permit not filled up for the last Cargo hose test carried out on 22 Feb 2019.","Documentation","Cargo / Ballast Systems","Inappropriate Procedure","8.62","Medium","","","The checklist was followed   for the next operations of pressure testing of cargo hose","2019-03-22","","Completed","2019-03-18","No","No","No","Internal"]
[null,null,null,null,9591,"46_Mon Jan 13 2020 10:09:55 GMT+0000","2019-03-16","Observation","Owner / Marine / Tech. Suptd.","Mooring Audit","Mooring winch brake stopper bolts to be adjusted present clearance less than 2 mm( Minimum required (5-6 mm)","Deck - Mooring Machinery","Mooring","Equipment Related","9.14","Medium","","","Brake bolts adjusted to 5mm as per the requirement.","2019-05-15","","Completed","2019-03-18","No","No","No","Internal"]
[null,null,null,null,5484,"46_25/10/2019 7:04:35 AM","2019-03-19","Defect","PSC Insp.","PSC Inspection","C/E and 3/E CRA was not able to presented to PSCO for verification at the point of inspection (both joined on 14/03/2019)","Documentation","Cert. & Docu.","Human Error,Inappropriate Procedure","3.5","Medium","Certificates & Documentation","","sMaster informed crewing department regarding the missing CRA and office immediately sent the copy of applied CRA prior completion of inspection and hence the inspector closed out the observation.","2019-03-19","","Completed","2019-03-19","No","No","No","External"]
[null,null,null,null,5485,"46_25/10/2019 7:08:47 AM","2019-03-19","Defect","PSC Insp.","PSC Inspection","The lifebuoy and the lifeboat retro reflective were found worn, torn and unable to stick in position","LSA / FFA","Safety / LSA / FFA","Human Error,Inappropriate Procedure","5.31","High","Life saving appliances","","The relevant retro reflective tape were immediately replaced and shown to the the PSCO prior completion of inspection","2019-03-19","","Completed","2019-03-19","No","No","No","External"]
[null,null,null,null,5486,"46_25/10/2019 7:15:07 AM","2019-03-19","Non Conformity","PSC Insp.","PSC Inspection","PSCO boarded the vessel by pilot ladder without any access control implement and proceed to officer dinning saloon alone, without anyone checking ID and verified before proceeding to Captain cabin, which is a serious breach of ISPS","Miscellaneous","ISPS Related","Human Error,Inappropriate Procedure","7.12","High","ISPS","","All ship staff were briefed by SSO about the security measures as per SSP and consequences of its Noncompliance.\n\n\n\nTraining and Safety comitee meeting carried out for the same and reports filed.\n\n\n\nInternal audit was conducted subsequent to this incident.","2019-03-20","","Completed","2019-03-20","No","No","No","External"]
[null,null,null,null,5487,"46_25/10/2019 7:27:50 AM","2019-03-20","Non Conformity","Owner / Marine / Tech. Suptd.","ISPS Audit","Various entries in the visitor's log were found incomplete for the last port of call. columns such as company, purpose of visit, time on, time off,and signature were not filled up for all visitors.","Miscellaneous","ISPS Related","Inappropriate Procedure","7.3","Low","","","correct and complete entries were made in the   next upcoming berth and entries verified and counter signed by the SSO.","2019-03-24","","Completed","2019-03-24","No","No","No","Internal"]
[null,null,null,null,5488,"46_25/10/2019 7:30:16 AM","2019-03-20","Non Conformity","Owner / Marine / Tech. Suptd.","ISPS Audit","refer to the email from hsqe date 29 nov 2018.As per the above email additional column was not made in the gangway log book for the alcohol /breath test to check the ship's crew returning from shore leave.","Documentation","ISPS Related","Inappropriate Procedure","7.3","Low","","","vessel has made the column for the BAC test for the all the pages of the visitors log  and instructed the crew to make the appropriate entries in the visitors log.","2019-03-24","","Completed","2019-03-24","No","No","No","Internal"]
[null,null,null,null,5489,"46_25/10/2019 7:33:01 AM","2019-03-26","Defect","Ship Staff","Ship Staff Insp.","PORT AND STBD ANCHOR SWIVEL WASTAGE DUE TO WHICH IT IS GETTING STUCK IN ONE POSITION AND NOT FREE TO MOVE.EVRYTIME IT HAS TO BE TURN MANUALLY AFTER USING THE ANCHOR.","Deck - Mooring Machinery","Mooring","Equipment Related","9.2","Very High","","","Deferred to D D","2019-03-30","","Completed","2019-08-15","No","No","No","Internal","Basis concurrence by Tech. Supt, this defect should be closed-out in this list & inserted in the dry-dock repairs spec. in Refman, c/w drawing / specifications. In the meantime, necessary precautions to be taken when manually turning the swivel after each operation."]
[null,null,null,null,5495,"46_2019-10-25 09:21:18.000","2019-04-02","Defect","Ship Staff","Ship Staff Insp.","NO.3 (S) COT DIGITAL INDICATOR SHOWING ZERO INDICATION.","Cargo Mach.,Hull & Tanks","Cargo / Ballast Systems","Equipment Related","8.19","Medium","","","Mussasino rechnician attended at singapore and replaced the sensor , same is working satisfactory now.","2019-04-30","WRUB190104","Completed","2019-04-18","No","No","No","Internal"]
[null,null,null,null,5543,"46_26/10/2019 11:59:32 AM","2019-04-05","Defect","Ship Staff","Ship Staff Insp.","Main Engine Jacket water cooler end cover to be renewed.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Replaced with newly received one, No leakages","2019-04-30","","Completed","2019-04-26","No","No","No","Internal"]
[null,null,null,null,5504,"46_26/10/2019 6:21:14 AM","2019-04-10","Defect","Ship Staff","Ship Staff Insp.","FOG HORM MOTOR LOW INSULATION","Navigation - Others","Navigation","Equipment Related","4.7","High","","","Motor over hauled, bearings renewed and installed in place, same working satisfactory now","2019-05-30","WRUB190126","Completed","2019-05-29","No","No","No","Internal"]
[null,null,null,null,5496,"46_2019-10-25 09:27:24.000","2019-04-11","Defect","Ship Staff","Ship Staff Insp.","BROKEN BLOCK IN ENGINE EMG ESCAPE TRUNK AND NO BLOCK FOR  PUMPROOM AND CARGO TANK RESCUE","LSA / FFA","Safety / LSA / FFA","Equipment Related,Human Error,Inappropriate Procedure","10.15","Low","","","Blocks received and renewed in all location","2019-04-30","WRUB190119","Completed","2019-04-24","No","No","No","Internal"]
[null,null,null,null,5500,"46_2019-10-25 09:55:53.000","2019-04-11","Defect","Ship Staff","Ship Staff Insp.","STAY WIRE OF FWD MAST AND MAIN MAST BROKE DURING HEAVY WEATHER.","Miscellaneous","General Appearance","Equipment Related,External Factors","11.3","Medium","","","Stay wire received & renewed","2019-04-30","WRUB190122","Completed","2019-04-29","No","No","No","Internal"]
[null,null,null,null,5505,"46_26/10/2019 6:28:20 AM","2019-04-11","Defect","Ship Staff","Ship Staff Insp.","BALLAST MANHOLE PACKING FOUND TO BE DETEREORATED MISSING IN SOME MANHOLES .","Deck - Pipe / Fittings","Cert. & Docu.","Equipment Related","11.3","Medium","","","New packing received and replaced","2019-06-30","WRUB190123","Completed","2019-06-10","No","No","No","Internal"]
[null,null,null,null,5497,"46_2019-10-25 09:32:46.000","2019-04-18","Defect","Class Surveyor","OM Insp. (Eg. SIRE / CDI etc.)","STBD SIDE LIFEBOAT WINCH BRAKE BRACKET THINNED DOWN","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.29","High","","","New bracket fabricated and replaced","2019-04-30","","Completed","2019-04-19","No","No","No","External"]
[null,null,null,null,5498,"46_2019-10-25 09:34:37.000","2019-04-18","Defect","Class Surveyor","OM Insp. (Eg. SIRE / CDI etc.)","SPRINKLER ON PORT AND STBD BOAT JAMMED","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.29","High","","","both sprinkler valves made free","2019-04-30","","Completed","2019-04-19","No","No","No","External"]
[null,null,null,null,5544,"46_26/10/2019 2:56:51 PM","2019-05-04","Defect","Ship Staff","Ship Staff Insp.","Aux Engine #1, Turbocharger washing arrangement is not correct ","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.12","Very High","","","Renewed and fitted in place.","2019-05-15","WRUB190035","Completed","2019-05-27","No","No","No","Internal"]
[null,null,null,null,5508,"46_26/10/2019 6:44:53 AM","2019-05-09","Defect","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","THE SELF IGNITING LIGHT OF THE LIFEBUOY LOCATED STARBOARD SIDE AFTER BOAT DECK WAS FOUND NOT WORKING. IT WAS RENEWED IMMEDIATELY","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.31","High","","","RECEIVED AND REPLACED","2019-07-30","WRUB190162","Completed","2019-07-22","No","No","No","External"]
[null,null,null,null,5545,"46_26/10/2019 3:06:38 PM","2019-05-09","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Deck AIr compressor was found to be working with alarm code 4805, it was cabinet air filter cloggy.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","filter changed with new one.","2019-05-10","","Completed","2019-05-09","No","No","No","Internal"]
[null,null,null,null,5507,"46_26/10/2019 6:41:59 AM","2019-05-13","Defect","Ship Staff","Ship Staff Insp.","6 FRAMO COFFERDAM PURGING NON- RETURN COUPLER STUCK AND RECOMMENDED TO REPLACE BY FRAMO TECHNITION","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.9","High","","","RECEIVED AND REPLACED","2019-07-30","WRUB190132","Completed","2019-07-22","No","No","No","Internal"]
[null,null,null,null,5532,"46_2019-10-26 09:17:54.000","2019-05-16","Defect","Ship Staff","Ship Staff Insp.","LIFEBOAT DOOR PACKING LEAKING ","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.29","High","","","DOOR PACKING RENEWED","2019-08-30","WRUB190169","Completed","2019-08-28","No","No","No","Internal"]
[null,null,null,null,7800,"46_Sat Oct 26 2019 10:06:42 GMT+0000 (Coordinated Universal Time)","2019-05-18","Defect","Ship Staff","Ship Staff Insp.","5 CARGO TANKDOME NEOPRINE PACKINGS NEED RENEWAL DUE TO DETERIORATION","Deck - Pipe / Fittings,Hull & Tanks","Cargo / Ballast Systems","Equipment Related","8.18","Low","","","replaced","2019-12-31","WRUB190166","Completed","2019-12-27","No","No","No","Internal"]
[null,null,null,null,7801,"46_Sat Oct 26 2019 10:10:05 GMT+0000 (Coordinated Universal Time)","2019-05-18","Defect","Ship Staff","Ship Staff Insp.","20 TANK CLEANING HATCH PACKING NEEDS RENEWAL","Deck - Pipe / Fittings,Hull & Tanks","Cargo / Ballast Systems","Equipment Related","8.18","Low","","","replaced","2019-12-31","WRUB190166","Completed","2019-12-27","No","No","No","Internal"]
[null,null,null,null,5538,"46_2019-10-26 10:06:42.000","2019-05-18","Defect","Ship Staff","Ship Staff Insp.","5 CARGO TANKDOME NEOPRINE PACKINGS NEED RENEWAL DUE TO DETERIORATION","Deck - Pipe / Fittings,Hull & Tanks","Cargo / Ballast Systems","Equipment Related","8.18","Low","","","replaced","2019-12-15","WRUB190166","Completed","2020-01-12","No","No","No","Internal","Requisition still in processing stage."]
[null,null,null,null,5539,"46_2019-10-26 10:10:05.000","2019-05-18","Defect","Ship Staff","Ship Staff Insp.","20 TANK CLEANING HATCH PACKING NEEDS RENEWAL","Deck - Pipe / Fittings,Hull & Tanks","Cargo / Ballast Systems","Equipment Related","8.18","Low","","","spare received in singapore and replaced","2019-12-15","WRUB190166","Completed","2019-12-27","No","No","No","Internal","Requisition still under processing stage."]
[null,null,null,null,5540,"46_2019-10-26 10:18:45.000","2019-05-23","Defect","Ship Staff","Ship Staff Insp.","SOME OF THE SOUNDING PIPE CAPS THREADS WORN OUT AND HENCE UNABLE TO LOCK","Hull & Tanks","Cargo / Ballast Systems","Equipment Related","8.18","Low","","","NEW SOUNDING CAP RECEIVED AND PLACED","2019-10-30","WRUB190159","Completed","2019-10-20","No","No","No","Internal"]
[null,null,null,null,5553,"46_26/10/2019 4:42:46 PM","2019-05-24","Defect","Ship Staff","Ship Staff Insp.","Emergency generator Exhaust pipe corroded and needs renewal.","Deck - Pipe / Fittings","Emgcy. Systems","Equipment Related","10.32","Very High","","","Fabricated and boxed back.","2019-08-30","","Completed","2019-07-22","No","No","No","Internal"]
[null,null,null,null,5506,"46_26/10/2019 6:34:39 AM","2019-05-25","Defect","Ship Staff","Ship Staff Insp.","4 FIRE DOOR NOT CLOSING PROPERLY, DOOR CLOSER IMPROPER OPERATION ","Accommodation","Safety / LSA / FFA","Equipment Related","5.35","Medium","","","Door closer received and replaced","2019-07-30","WRUB190160","Completed","2019-07-22","No","No","No","Internal"]
[null,null,null,null,5516,"46_26/10/2019 7:47:46 AM","2019-05-26","Defect,Non Conformity","Ship Staff","Ship Staff Insp.","2 FIRE HYDRANTS FOUND SLIGHTLY LEAKING IN CLOSED POSITION","LSA / FFA","Safety / LSA / FFA","Equipment Related,Inappropriate Procedure","5.35","Medium","","","Lapping carried out on all hydrants, 3 NEW HYDRANTS RECEIEVED PLANED TO REPLACE THE APROPRIATE VALVE","2019-08-30","","Completed","2019-08-12","No","No","No","Internal"]
[null,null,null,null,5528,"46_2019-10-26 08:47:25.999","2019-06-01","Defect","Ship Staff","Ship Staff Insp.","INDENTED AT TRANSVERSE BULKHEAD PLATING IN FR 150 SEC IN BETWEEN 7 TO 10 HORIZONTAL GIRDER AND CRACKED & BUCKLED IN 8 & 9 HORIZONTAL GINDER AT THE JOINED SEAM OF SIDE LONG. BHD. IN WBT 2P","Hull & Tanks","Structural Condn. / WT integrity ","External Factors","11.1","High","","","Deferred to D D","2019-08-30","","Completed","2019-08-30","No","No","No","Internal"]
[null,null,null,null,5517,"46_26/10/2019 7:57:11 AM","2019-06-04","Defect","Ship Staff","Ship Staff Insp.","WBT 3P:\n\n2. WBT 3P Localized Heavy Corrosion in welded Seam located Tank Side Bulkhead in Between Side Long. Bhd 12 & 11 and Fr 138 & 137 Sec in Fwd 2nd Compartment of No. 1st STR,\n\n3. WBT 3P Localized Heavy Corrosion located in Horizontal Ginder End Bracket of Fr 142 Sec at Side Long. Bhd No. 7 in Fwd 1st Compartment of No. 2nd STR,","Hull & Tanks","Structural Condn. / WT integrity ","External Factors","2.16","Medium","","","derusting and painting carried out.","2019-08-30","","Completed","2019-08-07","No","No","No","Internal"]
[null,null,null,null,5519,"46_2019-10-26 08:30:38.999","2019-06-04","Defect","Ship Staff","Ship Staff Insp.","WBT 4P:\n\n1. WBT 4P - 3 Spot Dent Coating Breakdown & Heavy Corrossion located in Side Shell Plate between Side Long. Bhd No. 12 & 11 Near Fr 124 Sec in 2nd Compartment of No.1st STR,\n\n2. WBT 4P - Localized Heavy Corrossion located in Side Shell Plate between Side Long. Bhd No. 12 & 10 Near Fr 128 Sec in 1st Compartment of No.1st STR,\n\n3. WBT 4P Slight Bent in Localized Heavy Corrosion located in Horizontal Ginder End Bracket of Fr 128 Sec at Side Long. Bhd No. 6 in 1st Compartment at No. 2nd STR, ","Hull & Tanks","Structural Condn. / WT integrity ","External Factors","2.16","Medium","","","derusting and painting completed","2019-08-30","","Completed","2019-08-07","No","No","No","Internal"]
[null,null,null,null,5520,"46_2019-10-26 08:32:03.000","2019-06-04","Defect","Ship Staff","Ship Staff Insp.","WBT 4S:\n\n5. WBT 4S - 63cm Edge Heavy Corrosion in Side Long. Bhd No. 13 in between  Fr 128 and 124 Sec Fwd 1st Compartment and No. 1st STR, .\n\n6. WBT 4S - 135cm Edge Heavy Corrosion in Side Long. Bhd No. 7 in bettween  Fr 116 and 120 Sec, Aft of 3rd Compartment and No. 2nd STR, \n\n7. WBT 4S - Coating Failure in new installed Side Shell Plate between Side Long. Bhd No. 6 & 10 Near Fr 116 Sec at 4th Compartment of No. 2nd STR, \n\n8. WBT 4S - Slight Bent in Localized Heavy Corrosion located in Horizontal Ginder End Bracket of FR 128 Sec at Side Long. Bhd No. 13, \n\n9. WBT 4S - Spot Coating Breakdwon and Heavy Corrosion in 2 Dent (10cmx10cm&12cmx10cm)in Side Shell in bet Side Long.Bhd No. 1&2, just above No.1 Near Fr 128 Sec at 1st Comp of Inn Bott, \n\n10. WBT 4S - Spot Coating Breakdwon and Heavy Corrosion in Dent in Side Shell in between Side Long. Bhd No. 7 & 8, just above No. 7 Near Fr 112 Sec  and 5th Compartment of No. 2nd STR, ","Hull & Tanks","Structural Condn. / WT integrity ","External Factors","2.16","Medium","","","derusting and painting completed","2019-08-30","","Completed","2019-08-07","No","No","No","Internal"]
[null,null,null,null,5521,"46_2019-10-26 08:33:45.999","2019-06-04","Defect","Ship Staff","Ship Staff Insp.","WBT 5P:\n\n1. WBT 5P Spot Dented and Coating Breakdown/Localized Corrosion located in Side Shell in between side long. Bhd No. 11 & 12 at 1st Compartment of No. 1st STR. (Fr 104-108 Sec), ","Hull & Tanks","Structural Condn. / WT integrity ","External Factors","2.16","Medium","","","derusting and painting completed","2019-08-30","","Completed","2019-08-07","No","No","No","Internal"]
[null,null,null,null,5522,"46_2019-10-26 08:35:04.000","2019-06-04","Defect","Ship Staff","Ship Staff Insp.","WBT 5S:\n\n1. WBT 5S  - Localized Coating Breakdown and slight corrosion located in Side Shell between Side Long. Bhd No. 11 & 12  at 5th Compartment of No.1st STR Near Fr 93 Sec., ","Hull & Tanks","Structural Condn. / WT integrity ","External Factors","2.16","Medium","","","derusting and painting completed","2019-08-30","","Completed","2019-08-07","No","No","No","Internal"]
[null,null,null,null,5523,"46_2019-10-26 08:36:17.000","2019-06-04","Defect","Ship Staff","Ship Staff Insp.","WBT 6P:\n\n1. WBT 6P - Localized Heaving Corrosion located in Side Shell between Side Long. Bhd No. 13 and 12 at 7th Compartment of 1st STR (Fr 63-59 Sec),\n\n2. WBT 6P - Localized Heaving Corrosion located in Side Shell between Side Long. Bhd No. 13 and 12 at 8th Compartment of 1st STR (Fr 63-59 Sec), \n\n","Hull & Tanks","Structural Condn. / WT integrity ","External Factors","2.16","Medium","","","derusting and painting completed","2019-08-30","","Completed","2019-08-07","No","No","No","Internal"]
[null,null,null,null,5524,"46_2019-10-26 08:38:26.000","2019-06-04","Defect","Ship Staff","Ship Staff Insp.","WBT 6S:\n\n1. WBT 6S - Localized Coating Breakdown & Corrosion located in Side Shell between Side Long. Bhd No. 14 and 15 at 7th Compartment of 1st STR (Fr 63-59 Sec), \n\n2. WBT 6S - Localized Coating Breakdown & Corrosion and 2 dented located in Side Shell between Side Long. Bhd No. 14 and 15 at 3rd Compartment of 1st STR (Fr 76-72 Sec), \n\n3. WBT 6S - Localized Coating Breakdown & Heavy Corrosion in Side Shell welded seam located in between Side Long. Bhd No. 7 and 6 at 7th Compartment of 2nd STR Near Fr 63 Sec,\n\n4. WBT 6S - Localized Edge Heavy Corrosion located in Side Shell Long. Bhd No. 8 at 7th Compartment of 2nd STR Near Fr 63 Sec, \n\n","Hull & Tanks","Structural Condn. / WT integrity ","External Factors","2.16","Medium","","","derusting and painting completed","2019-08-30","","Completed","2019-08-07","No","No","No","Internal"]
[null,null,null,null,5525,"46_2019-10-26 08:39:45.000","2019-06-04","Defect","Ship Staff","Ship Staff Insp.","WBT 7P:\n\n1. WBT 7P - Localized Heaving Corrosion & Coating Breakdown in Welded Seam located in Side Shell between Side Long. Bhd No. 13 and 12 at 4th Compartment of 1st STR  Near Fr 43 Sec, \n\n2. WBT 7P - Localized Heaving Corrosion located in Side Shell between Side Long. Bhd No. 12 and 11 at 4th Compartment of 1st STR  Near Fr 43 \n\n3. WBT 7P - Localized Heaving Corrosion located in Side Shell in Side Long. Bhd No. 11 at 5th Compartment of 1st STR  Near Fr 43 Sec and with slight deformation of Side Long Bhd No. 11 & Fr 43 Sec,\n\n4. WBT 7P - Localized Heaving Corrosion and deformation of Fr 40 Sec Bhd in between Side Long. Bhd No. 13 & 12 at 5th Compartment of 1st STR, \n\n5. WBT 7P - Localized Heaving Corrosion and deformation of Fr 40 Sec Bhd and side shell in between Side Long. Bhd No. 13 & 12 and indented End Joined Side Long Bhd No. 12 at 6th Compartment of 1st STR, \n\n","Hull & Tanks","Structural Condn. / WT integrity ","External Factors","2.16","Medium","","","derusting and painting completed","2019-08-30","","Completed","2019-08-07","No","No","No","Internal"]
[null,null,null,null,5527,"46_2019-10-26 08:40:55.000","2019-06-04","Defect","Ship Staff","Ship Staff Insp.","WBT 7S:\n\n1. WBT 7S - Localized Corrosion & Coating Breakdown located in Side Shell between Side Long. Bhd No. 12 and 11 at 6th Compartment of 1st STR (Fr 40-37 Sec), ","Hull & Tanks","Structural Condn. / WT integrity ","External Factors","2.16","Medium","","","derusting and painting completed","2019-08-30","","Completed","2019-08-07","No","No","No","Internal"]
[null,null,null,null,5518,"46_26/10/2019 7:59:14 AM","2019-06-09","Defect","Ship Staff","Ship Staff Insp.","WBT 3S:\n\n2. WBT 3S - 1 Spot Dent Coating Breakdown & Heavy Corrossion located in between Side Shell Long. Bhd No. 13 & 12  Near Fr 135 Sec in 2nd Compartment of No.1st STR,\n\n3. WBT 3S - 1 Spot Dent Coating Breakdown & Heavy Corrossion located in Side Shell Plate Top of Side Long. Bhd No. 11 Near Fr 128 Sec in 4th Compartment of No.1st STR,\n\n4. WBT 3S Localized Heavy Corrosion in Welded Beads located in Side Long. Bhd No. 13 Near of Fr 128 Sec in 4th Compartment at No. 1st STR, \n\n","Hull & Tanks","Structural Condn. / WT integrity ","External Factors","2.16","Medium","","","derusting and painting carried out","2019-08-30","","Completed","2019-08-07","No","No","No","Internal"]
[null,null,null,null,5535,"46_2019-10-26 09:37:18.000","2019-06-19","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Pressure test old common line manifold valve","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.41","Very High","","","Pressure tested. in order","2019-09-15","","Completed","2019-10-08","No","No","No","Internal"]
[null,null,null,null,7019,"46_Sat Oct 26 2019 09:05:18 GMT+0000 (Coordinated Universal Time)","2019-06-30","Defect","Ship Staff","Ship Staff Insp.","FIRE DOOR NEAR CREW LAUNDRY TEMPORARY REPAIRED BUT NEEDS RENEWAL DUE TO CRACK AT BASE","Accommodation,LSA / FFA","Safety / LSA / FFA","Equipment Related","5.35","Medium","","","Deferred to D D","2019-08-30","","Completed","2019-08-06","No","No","No","Internal"]
[null,null,null,null,5529,"46_2019-10-26 09:05:18.000","2019-06-30","Defect","Ship Staff","Ship Staff Insp.","FIRE DOOR NEAR CREW LAUNDRY TEMPORARY REPAIRED BUT NEEDS RENEWAL DUE TO CRACK AT BASE","Accommodation,LSA / FFA","Safety / LSA / FFA","Equipment Related","5.35","Medium","","","NEW FIRE DOOR RECEIVED AT SINGAPORE ON 30TH JUNE 2020. FIRE DOOR REPLACED.","2020-07-30","WRUB200021","Completed","2020-07-08","Yes","No","No","Internal","doors ordered, will be replaced in DD"]
[null,null,null,null,5555,"46_26/10/2019 4:49:33 PM","2019-07-19","Defect","Ship Staff","Ship Staff Insp.","ME funnel wire repair to be done at suitable Anchorage.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Temporary repair have been carried out by ship staff.","2019-08-30","","Completed","2019-09-30","Yes","No","No","Internal"]
[null,null,null,null,5552,"46_26/10/2019 4:24:11 PM","2019-07-20","Defect","Ship Staff","Ship Staff Insp.","Accomodation AC Compressor No.1 found abnormal sound and vibration.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","AC replaced with new one. All test carried out and working satisfactory. No leakages.","2019-07-30","","Completed","2019-07-22","No","No","No","Internal"]
[null,null,null,null,5526,"46_2019-10-26 08:44:34.000","2019-07-29","Defect","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","The brake linings of five mooring winches (fore port outer, fore starboard outer, aft port two & aft starboard inner) located in the Fore & Aft mooring station were found thinned down and damaged at 5 locations. (VIQ 9.15).","Deck - Mooring Machinery","Mooring","Equipment Related,Inappropriate Procedure","9.15","Medium","","","all mooring winches brake linings changed and brake rendering test carried out.","2019-08-30","","Completed","2019-08-13","No","No","No","External"]
[null,null,null,null,9667,"46_15/1/2020 9:02:06 PM","2019-07-29","Observation","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","Handrails or other handholds were not provided in corridors inside the accomodation block.","Accommodation","General Appearance","Inappropriate Procedure","11.13","Low","","","newly installed handrails in all the alleyways","2019-09-01","","Completed","2019-08-08","No","No","No","External"]
[null,null,null,null,5450,"46_2019-10-26 10:21:01.999","2019-07-30","Defect","Ship Staff","Ship Staff Insp.","2S COT PUMP STACK CALMPS ON TEMP SENSORS AND DISCH LINE MISSING.","Cargo Mach.,Deck - Pipe / Fittings,Hull & Tanks","Cargo / Ballast Systems","Equipment Related","8.18","Low","","","STAGING REQUIRED TO RETIFY SAME, AS ALL ARE ABOVE 8 MTR HEIGHT. Can not be carried out with ship's crew as job require stagging. Request to put the job in refman for drydock","2020-03-20","","Completed","2020-10-19","Yes","No","No","Internal","Please include the job in DD."]
[null,null,null,null,7020,"46_Sat Oct 26 2019 09:09:54 GMT+0000 (Coordinated Universal Time)","2019-07-30","Defect","Ship Staff","Ship Staff Insp.","FW LINE AND AIR LINE ON DECK HEAVILY CORODED WITH MULTIPLE SOFT PATCHES.","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.4","Very High","","","Deferred to D D","2019-08-30","","Completed","2019-08-06","No","No","No","Internal"]
[null,null,null,null,7802,"46_Sat Oct 26 2019 10:30:21 GMT+0000 (Coordinated Universal Time)","2019-07-30","Defect","Ship Staff","Ship Staff Insp.","MULTIPLE SUPPORT BARS FOR GRATINGS ON CATWALK  BROKEN AND NEEDS RENEWAL","Miscellaneous","General Appearance","Equipment Related,External Factors","11.3","Medium","","","Support bar derusted, fixed with nut & bolts.","2020-03-30","","Completed","2020-07-25","Yes","No","No","Internal"]
[null,null,null,null,5531,"46_2019-10-26 09:14:19.999","2019-08-03","Breakdown,Defect","Ship Staff","Ship Staff Insp.","port side gangaway winch motor not working due to rotor damage","Deck - Machinery","General Appearance","Equipment Related","5.47","Low","","","winch motor replaced","2019-08-30","WRUB190210","Completed","2019-08-19","No","No","No","Internal"]
[null,null,null,null,5534,"46_2019-10-26 09:34:36.000","2019-08-06","Defect","Ship Staff","Ship Staff Insp.","Both anchor windlass brake liners thinned down need to renew. ","Deck - Mooring Machinery","Mooring","Equipment Related","9.15","Medium","","","windlass brake liner renewed","2019-10-06","WRUB190222","Completed","2019-10-03","No","No","No","Internal"]
[null,null,null,null,5448,"46_26/10/2019 3:23:13 PM","2019-08-25","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Attened Deck Air Compressor alarm A0085 same to be reset","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Filter cleaned and timer is reset. No alarm at present.","2019-08-27","","Completed","2019-08-27","No","No","No","Internal"]
[null,null,null,null,5509,"46_26/10/2019 6:54:41 AM","2019-08-25","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","2 no’s rollers to be freed on poop deck aft","Deck - Mooring Machinery","Mooring","Equipment Related,Inappropriate Procedure","9.18","Low","","","ROLLERS OPENED AND GREASED. MADE FREE TO ROTATE","2019-09-01","","Completed","2019-09-22","No","No","No","Internal"]
[null,null,null,null,5510,"46_26/10/2019 6:58:31 AM","2019-08-25","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Accommodation ladder side Roller to be freed","Deck - Machinery","General Appearance","Equipment Related,Inappropriate Procedure","5.47","Low","","","SIDE ROLLERS MADE FREE TO ROTATE","2019-09-09","","Completed","2019-09-07","No","No","No","Internal"]
[null,null,null,null,5511,"46_26/10/2019 7:01:10 AM","2019-08-25","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Pressure gauge 9P COT tank glass broken, to renew.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.13","Low","","","REPLACED WITH SPARE ONBOARD","2019-08-27","","Completed","2019-08-27","No","No","No","Internal"]
[null,null,null,null,5512,"46_26/10/2019 7:04:21 AM","2019-08-25","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","All common spaces Toilet bowl to be cleaned & urinal to be cleared.","Accommodation","General Appearance","Behaviour Based,Inappropriate Procedure","11.13","Low","","","CLEANED AND MAINTAINED",null,"","Completed","2019-08-29","No","No","No","Internal"]
[null,null,null,null,5513,"46_26/10/2019 7:37:35 AM","2019-08-25","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Life boat deck - Emergency Light - Stbd & Port: To free the light arms which are frozen in their present positions.","LSA / FFA","Safety / LSA / FFA","Behaviour Based,Inappropriate Procedure","11.5","Medium","","","LIGHT POST FREE AND CLEAR SWINGING","2019-08-28","","Completed","2019-08-28","No","No","No","Internal"]
[null,null,null,null,5514,"46_26/10/2019 7:40:03 AM","2019-08-25","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Hospital (a) Find the source of foul smell and fix it and (b) To repair the bathroom door lock, which cannot be closed from inside.","Accommodation","General Appearance","Inappropriate Procedure","11.15","Low","","","Idendified source, cleaned and foul smell observed, door lock repaired","2019-08-31","","Completed","2019-09-11","No","No","No","Internal"]
[null,null,null,null,5515,"46_26/10/2019 7:45:13 AM","2019-08-25","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Hyd valve stands on deck, to operate ballast valves do not have marking to indicate OPEN and SHUT position of the ballast valve.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Human Error,Inappropriate Procedure","8.21","Medium","","","marking done","2019-09-25","","Completed","2019-09-08","No","No","No","Internal"]
[null,null,null,null,5536,"46_2019-10-26 09:39:32.000","2019-08-25","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","2 in number spare 150A new cargo manifold valve to replace with leaking one","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.41","Very High","","","new 150A cargo valve fitted and pressure tested","2019-09-25","","Completed","2019-10-11","No","No","No","Internal"]
[null,null,null,null,5547,"46_26/10/2019 3:17:25 PM","2019-08-25","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Emergency generator exhaust pipe lagging missing","E/R - Aux. Engine","Emgcy. Systems","Equipment Related","10.32","Very High","","","Lagging fixed in place.","2019-08-29","","Completed","2019-08-28","No","No","No","Internal"]
[null,null,null,null,5548,"46_26/10/2019 3:26:36 PM","2019-08-25","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Main air compressor No.1 attached coolind pump seal leakage.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Seal repalced with spare new one. At present no leakage.","2019-09-02","","Completed","2019-08-29","No","No","No","Internal"]
[null,null,null,null,5549,"46_26/10/2019 4:04:48 PM","2019-08-25","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Tablet dosing chart to be placed near the sewage treatment plant. Dosing cap thread area to be repaired.","E/R - Aux. Mach.","Emgcy. Systems","Equipment Related","10.32","Very High","","","Job completed","2019-08-27","","Completed","2019-08-27","No","No","No","Internal"]
[null,null,null,null,5550,"46_26/10/2019 4:11:24 PM","2019-08-25","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","All sea water pipe are rusted and salt deposits. Desalt and paint is required to be done.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","cleaning and painting carried out.","2019-08-29","","Completed","2019-08-28","No","No","No","Internal"]
[null,null,null,null,5551,"46_26/10/2019 4:15:53 PM","2019-08-25","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ME lube oil purifier steam return line chocked, needs to be cleared.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","cleaning carried out.","2019-09-09","","Completed","2019-09-02","No","No","No","Internal"]
[null,null,null,null,7807,"46_Sat Oct 26 2019 10:37:19 GMT+0000 (Coordinated Universal Time)","2019-09-19","Defect","Ship Staff","Ship Staff Insp.","ME air cooler sea water inlet pipe corroded","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","PIPELINE FABRICATED WITH NEW FLANGE , TRIED OUT WORKING SATISFACTORY . JOB COMPLETED .","2019-12-15","WRUB190247","Completed","2019-11-29","No","No","No","Internal"]
[null,null,null,null,5542,"46_2019-10-26 10:37:19.999","2019-09-19","Defect","Ship Staff","Ship Staff Insp.","ME air cooler sea water inlet pipe corroded","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Pipe renewed","2019-12-15","WRUB190247","Completed","2019-12-30","No","No","No","Internal","."]
[null,null,null,null,5556,"46_26/10/2019 4:53:49 PM","2019-09-24","Defect","Ship Staff","Ship Staff Insp.","While discharging Cargo in Port Qasim, 3S Cargo pump remote control valve started leaking due to wear and tear of Block valve body tightening thread.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.16","Medium","","","Spare new valve received on 12th Oct, same was replaced with old one. Test carried out and all found satisfactory.At present no leakages.","2019-10-15","wrub190248","Completed","2019-10-12","No","No","No","Internal"]
[null,null,null,null,7803,"46_30/11/2019 4:38:17 PM","2019-10-06","Defect","Ship Staff","Ship Staff Insp.","The MDS laptop onboard is used for on board chart correction and ENC ordering. There is problem in accessing the UKHO website and also had hard disk problem.","Navigation - Others","Navigation","Equipment Related","4.12","Very High","","","RECTIFIED","2019-12-08","","Completed","2020-01-11","No","No","No","Internal"]
[null,null,null,null,5712,"46_31/10/2019 6:53:11 AM","2019-10-29","Defect","Ship Staff","Ship Staff Insp.","Stbd manifold framo emergency stop box frame broken from the railing due to corroision","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.1","Very High","","","New wooden frame made for framo emergency stop box and fixed on the railings.","2019-11-01","","Completed","2019-10-29","No","No","No","Internal"]
[null,null,null,null,5711,"46_31/10/2019 6:57:49 AM","2019-10-30","Defect","Ship Staff","Ship Staff Insp.","Both anchor additional lashing wire found few strand broken\t","Deck - Mooring Machinery","Mooring","Equipment Related,External Factors","9.2","Very High","","","Lashing wire received at singapore anchorage and replaced.","2019-11-15","WRUB190268","Completed","2019-11-14","No","No","No","Internal","Requisition under processing."]
[null,null,null,null,7809,"46_13/12/2019 8:02:59 PM","2019-11-14","Defect","Owner / Marine / Tech. Suptd.","Nav Audit / Verification","while at anchor, anchor ball displayed from forward mast was not clearly visible","Navigation - Others","Navigation","Inappropriate Procedure","4.7","High","","","lanyard replaced by long length. Hoist where it can best be seen","2019-11-15","","Completed","2019-11-14","No","No","No","Internal"]
[null,null,null,null,7021,"46_26/11/2019 11:37:19 AM","2019-11-18","Defect","Ship Staff","Ship Staff Insp.","Bunker line starboard valve operating mechanism found stuck .","Cargo Mach.","Cargo / Ballast Systems","Equipment Related,Inappropriate Procedure","6.21","High","","","Operating mechanism overhauled working satisfactory","2019-11-20","","Completed","2019-11-19","No","No","No","Internal"]
[null,null,null,null,7804,"46_30/11/2019 7:00:13 PM","2019-11-21","Defect","Ship Staff","Ship Staff Insp.","Crew laundry room dryier machine belt broken.","Elect. Mach. & Equip.","MLC Related","Equipment Related","11.16","Low","","","replaced with new belt and now operational","2019-12-25","WRUB190283","Completed","2019-12-27","No","No","No","Internal"]
[null,null,null,null,7806,"46_30/11/2019 4:58:16 PM","2019-11-30","Defect","Ship Staff","Ship Staff Insp.","Ballast line up valve no 27's Valve gear assembly broken and was unable to operate valve.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.21","Medium","","","replaced by old valve gear assembly and working satisfactory.","2019-11-30","","Completed","2019-11-30","No","No","No","Internal"]
[null,null,null,null,7810,"46_13/12/2019 7:56:48 PM","2019-12-10","Defect","Ship Staff","Ship Staff Insp.","Tank cleaning machine of 10s COT was not functional.\t\t\t\t\t\t","Deck - Machinery","Cargo / Ballast Systems","Equipment Related","8.8","Very High","","","overhauled and oil filled now operational","2019-12-12","","Completed","2019-12-10","No","No","No","Internal"]
[null,null,null,null,7811,"46_Sun Dec 15 2019 09:08:02 GMT+0000 (Coordinated Universal Time)","2019-12-10","Defect","Ship Staff","Ship Staff Insp.","Common line cross over valce 250A was found leaking.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.11","Medium","","","COMMON LINE CROSS OVER VALVE  GEAR ALIGNED AND OVERHAULED. PRESSURE TESTED. NO LEAKS.","2019-12-17","","Completed","2019-12-12","No","No","No","Internal"]
[null,null,null,null,7805,"46_Thu Dec 12 2019 18:35:36 GMT+0000 (Coordinated Universal Time)","2019-12-12","Defect","Ship Staff","Ship Staff Insp.","Boiler water control valve found leaking from gland .","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","11.12","Low","","","NEW GLAND FITTED . CONTROLLER TRIED OUT WORKING SATISFACTORY ","2019-12-25","","Completed","2019-12-24","No","No","No","Internal"]
[null,null,null,null,7808,"46_Thu Dec 12 2019 18:46:59 GMT+0000 (Coordinated Universal Time)","2019-12-12","Defect","Ship Staff","Ship Staff Insp.","Carolifier heating element found leaking","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","11.12","Low","","","C alorifier dismental , all gaskets renewed , calorifier pressure tested and fitted back , working satisfactory .","2019-12-16","","Completed","2019-12-13","No","No","No","Internal"]
[null,null,null,null,9651,"46_15/1/2020 8:15:32 PM","2020-01-07","Observation","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","The Flag state processing certificate (CRA) of endorsement for the on board 3rd Engineer was valid until 06-Dec-2019.A Scanned copy of the full term flag station licence, that was issued on 29-Oct-2019 was available on board.","Documentation","Cert. & Docu.","External Factors","3.5","Medium","","","The company office was informed and the documents delivered at vessels next port of call","2020-02-07","","Completed","2020-01-16","No","No","No","External"]
[null,null,null,null,9652,"46_15/1/2020 8:38:42 PM","2020-01-07","Observation","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","The ship Design MBL was 42.0 MT. The mooring ropes on the winches had their LDBF between 45.2 T to 50.5 T which corresponded to values greater than 108 % of the ship design MBL","Deck - Mooring Machinery","Mooring","Equipment Related","9.5","High","","","when ordering the rope, the LDBL of the rope should be less than a winch MBL. new ropes to be ordered accordingly, present condition of ropes satisfactory","2020-07-06","","Completed","2020-01-16","No","No","No","External"]
[null,null,null,null,9663,"46_15/1/2020 8:19:52 PM","2020-01-07","Observation","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","The daily position were not being logged in GMDSS radio log. On all the occasion in the last one month that were reviewed, the on load value of the batteries were being logged as higher than the off load value. Eg: On 04-Jan-2020 the On load/ Off load value were logged as 26.2V / 25.2 V.","Navigation - GMDSS & Communication","Navigation","Human Error","4.23","High","","","Training given to all deck officers that all entries should be as per VIQ 7.0.07 and as per the GMDSS logbook cover page. The offload and on load value reading should be precise and offload value should be higher than the on load value.","2020-02-07","","Completed","2020-01-09","No","No","No","External"]
[null,null,null,null,9664,"46_15/1/2020 8:26:33 PM","2020-01-07","Observation","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","For the Hot work carried out on 15-Apr-2019 and 16-apr-2019 on the sunken deck STBD side there were no record for the times and result of atmosphere monitoring during the hot work (Ref.ISGOTT section 9.4). Initial atmosphere checks had been carried out on both the above occasions.","Deck - Pipe / Fittings","Safety / LSA / FFA","Inappropriate Procedure","5.24","Very High","","","Additional page was included, times and result of atmosphere checks has been logged down. All ship staffs were trained for the requirements of atmosphere checks during hot work.","2020-02-06","","Completed","2020-01-07","No","No","No","External"]
[null,null,null,null,9645,"46_15/01/2020 4:45:29 PM","2020-01-13","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Lifebuoy grab line thinned down, to be replaced with new 9.5 mm rope. Order & replace with new rope","LSA / FFA","Safety / LSA / FFA","Inappropriate Procedure","5.31","High","","","9.5 mm Rope received onboard ship. replaced.","2020-01-31","WRUB200003","Completed","2020-02-16","No","No","No","Internal","Will expedite"]
[null,null,null,null,9646,"46_15/01/2020 4:59:19 PM","2020-01-13","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","No.2 DG T/C performance not satisfactory, T/C to be cleaned with carbon remover & check for performance","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","T/C dismanteled and kept in carbon remover. T/C boxed back with new bearing and seal rings . Clearances checked all with in limits . T/C preformance checked found satisfactory","2020-01-25","","Completed","2020-01-16","No","No","No","Internal","Please revert back once done"]
[null,null,null,null,9647,"46_15/01/2020 5:02:00 PM","2020-01-13","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Requisitions for DD specs to be made as discussed on board","Documentation","Cert. & Docu.","Inappropriate Procedure","10.32","Very High","","","Requsition for DD specs completed","2020-01-31","","Completed","2020-02-16","No","No","No","Internal"]
[null,null,null,null,9648,"46_15/01/2020 5:20:33 PM","2020-01-13","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ME No.5 exhaust temp on higher side compared to other units, exhaust v/v to be overhauled at first available opportunity","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Waiting for opportunity. Spare exhaust valve is ready to use","2020-02-15","","Completed","2020-07-17","No","No","No","Internal","please carry out first available opportunity"]
[null,null,null,null,9649,"46_15/01/2020 5:28:23 PM","2020-01-13","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","EGB bellow slightly leaking, dimension to be taken & DD specs to be made","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","DD specs raised and dimension taken","2020-01-15","","Completed","2020-01-26","No","No","No","Internal"]
[null,null,null,null,9650,"46_15/01/2020 5:38:46 PM","2020-01-13","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Vessel not able to find load cell supplied recently on board, same to searched dedicated place to be made for keeping in CCR. On board load test of chain blocks to be carried out & proper certificate to be made","Miscellaneous","Communication","Inappropriate Procedure","","","","","\n\nVessel found the load cell in N2 generator room.\n\n","2020-01-31","","Completed","2020-03-26","No","No","No","Internal"]
[null,null,null,null,9653,"46_15/01/2020 3:27:32 PM","2020-01-13","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","CRA of 2nd officer also about to expire, same to be connected at next port along with 3rd engineer CRA. Ask FPD to connect both certificate at next Sohar","Documentation","Cert. & Docu.","Human Error","3.5","Medium","","","Document received in Sohar Port. ","2020-01-25","","Completed","2020-01-13","No","No","No","Internal"]
[null,null,null,null,9654,"46_15/01/2020 3:33:33 PM","2020-01-13","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","UKC was shown as less than 1 at all the Legs which is incorrect.\n\nWatch level was not mentioned correctly in Plan.\n\nUKC not mentioned at anchorage or at berth in passage planning.\n\nCorrect the same & train the officer accordingly for future planning\n\n","Documentation","Navigation","Human Error","4.5","Very High","","","Coorection carried ut. Training part implemented. At present all officers are well aware of procedure to be followed.","2020-01-20","","Completed","2020-01-15","No","No","No","Internal"]
[null,null,null,null,9655,"46_15/01/2020 3:39:09 PM","2020-01-13","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Deck Logbook\n\nWatch keeping levels were not properly entered. When pilot on board still the level was being show as 3 & not upgraded to 4.\n\nHand steering engagement position not mentioned in Logbook.\n\nCorrect the same & train the officer accordingly for future recording     \n\n","Documentation","Cert. & Docu.","Human Error","4.2","Medium","","","Correction carried out. Officers training carried out. At present all officers are well aware of entry to be made in log book","2020-01-20","","Completed","2020-01-13","No","No","No","Internal"]
[null,null,null,null,9656,"46_15/01/2020 4:24:24 PM","2020-01-13","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","GMDSS log\n\nLogbook filled inappropriately & very shabbily ,,To be filled as per \n\nas per VIQ requirement, training to officer provided accordingly\n\n","Documentation","Cert. & Docu.","Human Error","4.23","High","","","Logbook to be filled neat and tidy. Explained to all officers. Training given to all officers","2020-01-20","","Completed","2020-01-17","No","No","No","Internal"]
[null,null,null,null,9657,"46_15/01/2020 4:34:18 PM","2020-01-13","Observation","Owner / Marine / Tech. Suptd.","Ship Staff Insp.","3 COT high level alarms & 2 overfill alarm were activated during inspection even tank level were less than 50% capacity. Sensors to be taken out & clean for possible sludge","Deck - Machinery","Cargo / Ballast Systems","Equipment Related","8.14","Medium","","","Sensor removed from the place after complete discharge of tank, precausions taken. Wet oil found on the sensor body. Cleaned and boxed back. Tried out, found working satisfactory.","2020-01-30","","Completed","2020-01-15","No","No","No","Internal"]
[null,null,null,null,9658,"46_15/01/2020 4:49:10 PM","2020-01-13","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Engine room ORB last weekly entry procedure missed out by CE & at occasion of bunkering entry in ORB 2 line item (26.1 & 26.2 were entered in single line instead of 2 separate lines) ","Documentation","Cert. & Docu.","Human Error","2.1","Very High","","","Missed entry carried out under section \" I \"","2020-01-20","","Completed","2020-01-15","No","No","No","Internal"]
[null,null,null,null,9659,"46_15/01/2020 5:06:25 PM","2020-01-13","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","No.1 HFO purifier safety coupling breaking regularly, to open purifier & check for cause","E/R - Purifier","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Purifier outlet pipe found chocked, bowl was having sludge. Same cleaned. Running satisfactory. Now in use.","2020-01-25","","Completed","2020-01-15","No","No","No","Internal"]
[null,null,null,null,9660,"46_15/01/2020 5:52:18 PM","2020-01-13","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Crew mess room curtains are very dirty, same to be taken out & washed.","Accommodation","General Appearance","Inappropriate Procedure","11.13","Low","","","Washing carried out. Now it is in clean condition.","2020-01-25","","Completed","2020-01-15","No","No","No","Internal"]
[null,null,null,null,9661,"46_15/01/2020 5:25:57 PM","2020-01-13","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","No.2 boiler water circulating pp seal leaking, same to be investigated & rectified","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Gland tightening studs bolt found worn out, same renewed. Complete gland packing replaced with new one. No leakages.","2020-01-25","","Completed","2020-01-15","No","No","No","Internal"]
[null,null,null,null,9662,"46_15/01/2020 5:56:37 PM","2020-01-13","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Area behind N2 plant has a lot of garbage, same to be cleared & arranged","Miscellaneous","General Appearance","Inappropriate Procedure","11.13","Low","","","Garbage removed and area cleaned.","2020-01-25","","Completed","2020-01-14","No","No","No","Internal"]
[null,null,null,null,9665,"46_15/01/2020 4:29:15 PM","2020-01-13","Observation","Owner / Marine / Tech. Suptd.","Ship Staff Insp.","Lifeboat bottles were not fully charged during time of inspection, one of the bottles pressure were less than 185 bar which is below the minimum required limits","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.28","Very High","","","Life boat bottle and pipe line checked for leakages. No leakages found, all satisfactory. Bottle charged with air. At present bottle pressure is 200 Bar.","2020-01-20","","Completed","2020-01-14","No","No","No","Internal"]
[null,null,null,null,9668,"46_15/01/2020 4:55:43 PM","2020-01-13","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","BRC load test% for all winches is being calculated on 55% as per formula/calculation which is less than requirement of 60%, same to be discussed with ops & corrected","Deck - Machinery","Mooring","Inappropriate Procedure","9.7","Medium","","","rendering test carried out at 60%","2020-01-25","","Completed","2020-01-16","No","No","No","Internal"]
[null,null,null,null,10349,"46_28/01/2020 7:03:43 PM","2020-01-20","Defect","Ship Staff","Ship Staff Insp.","Sea water service pump not developing pressure","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","pump spare recived in singapore . pump complete overhauling carrier out . tried out pump working satisfactoy.","2020-02-15","WRUB200004","Completed","2020-03-27","No","No","No","Internal"]
[null,null,null,null,10350,"46_28/1/2020 7:15:55 PM","2020-01-27","Defect","Ship Staff","Ship Staff Insp.","7S cot Framo pump rpm guage was found cracked","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.8","Very High","","","replaced with spare new guage","2020-02-15","","Completed","2020-01-27","No","No","No","Internal"]
[null,null,null,null,16858,"46_19/12/2020 4:19:37 PM","2020-02-17","Non Conformity","Ship Staff","Ship Staff Insp.","FWD STATION LIGHT UNLIT DURING MOORING OPERATIONS IN NIGHT HOURS","Miscellaneous","General Appearance","Knowledge Based","11.9","Low","","","Light was replaced with spare onboard. Advised to Person incharged before arrival port all lights ondeck to be check prior arrival.","2020-02-18","","Completed","2020-02-17","No","No","No","Internal"]
[null,null,null,null,12272,"46_15/03/2020 4:45:55 AM","2020-03-08","Defect","Ship Staff","Ship Staff Insp.","HYDRAULIC POWER PACK COOLER  SEA WATER OUTLET PIPE LEAKING ","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","SYSETM STOPED , COOLER SEA WATER LINE ISOLATED , PIPE REMOVED AND NEW PIPE FABRICATED . NEW PIPE BOXED BACK WORKING SATISFACTORY .","2020-03-09","","Completed","2020-03-09","No","No","No","Internal"]
[null,null,null,null,12273,"46_16/3/2020 7:26:29 PM","2020-03-10","Defect","Ship Staff","Ship Staff Insp.","6P 6S Manifold valve stbd side not holding","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.11","Medium","","","Both the valve replaced by spare overhauled valves.","2020-03-17","","Completed","2020-03-11","No","No","No","Internal"]
[null,null,null,null,12275,"46_16/3/2020 7:31:24 PM","2020-03-11","Defect","Ship Staff","Ship Staff Insp.","Ballast Valve no 24 in pump room difficult to close and open","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.11","Medium","","","valve removed and overhauled.","2020-03-25","","Completed","2020-03-12","No","No","No","Internal"]
[null,null,null,null,12274,"46_16/3/2020 7:36:07 PM","2020-03-14","Defect","Ship Staff","Ship Staff Insp.","cargo heating line mast steam valve for 1w,3w,9w not holding ","Deck - Pipe / Fittings","","Equipment Related","8.15","Medium","","","replaced by spare new valves","2020-03-25","","Completed","2020-03-14","No","No","No","Internal"]
[null,null,null,null,16859,"46_17/12/2020 4:11:57 PM","2020-03-20","Non Conformity","Ship Staff","Ship Staff Insp.","Unreported used of eye wash in engine room work shop found in open position (Eye wash Bottle is one time used)","Miscellaneous","Safety / LSA / FFA","Knowledge Based","5.46","Medium","","","Eye wash bottle replace with new one. All crew briefed once eye wash bottle used immediately inform 2nd Officer for replacement and advised to 2nd officer to carry out frequent rounds to check all eye wash bottle condition to adhere accordingly. ","2020-03-31","","Completed","2020-03-28","No","No","No","Internal"]
[null,null,null,null,12271,"46_30/03/2020 7:30:17 PM","2020-03-30","Defect","Ship Staff","Ship Staff Insp.","main engine preformance checking equipment doctor not able to store data . messahe showing data corrupted .","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","REPAIE CARRIED OUT ONBOARD . DOCTOR EQUIPMENT TRY OUT .WORKING SATISFACTORY","2020-05-01","","Completed","2020-05-16","No","No","No","Internal","repairs were carried out onboard"]
[null,null,null,null,14595,"46_14/04/2020 6:03:07 AM","2020-04-10","Breakdown,Observation","Ship Staff","Ship Staff Insp.","While maneuvering on 10th April 2020,ME exhuast temp was found increasing in Half ahead condition\n\nmore then 400 deg. Generaly it never increase more then 340 deg to 350 deg. Same time Amp checked for ME Aux blower, \n\nBlower No # 1 was showing 5 amps which is less, it should be 15amps. Blower No # 2 was showing 15 Amps.\n\nSuspected with belt and checked after maneuvering.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Belt for both blower and pully found in good condition. \n\nSuspected with impeller. Scavenge space ventilation carried out and man entry done after filling entry permit in scav space. \n\nNo 1 Blower impeller found broken from the boss as per mentioned in the manual. Same was cracked before my tenure.\n\nReplaced with new one and clerance between impeller and difuser found as per manual. Manual start checks carried out and Amp found satisfactory.\n\nNo vibration and abnormal sound. All satiafactory.\n\n","2020-04-11","","Completed","2020-04-11","No","No","No","Internal"]
[null,null,null,null,14596,"46_15/04/2020 4:24:48 PM","2020-04-13","Defect","Ship Staff","Ship Staff Insp.","OWS DISCHARGE PIPE BEFORE THREE WAY VALVE WAS HAVING PIN HOLE , SMALL AMOUNT OF WATER LEAKING WHEN OWS OPERATED .","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","INFORMED COMPANY , REMOVED THAT SECTION OF PIPE AFTER BREAKING SEALS . REPAIR CARRIED OUT AND PIPE  FITTED BACK . NEW SEALS WAS PUT ON RESPECTIVE FLANGE AND ENTRY MADE IN OWS SEAL LOG.","2020-04-15","","Completed","2020-04-15","No","No","No","Internal"]
[null,null,null,null,14597,"46_06/05/2020 3:59:09 PM","2020-04-13","Defect","Ship Staff","Ship Staff Insp.","2P CARGO PUMP NOT WORKING","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","INFORM ENGINE ROOM , PUMP WAS OPENNED AND INSPECTED , FOUND ONE BROKEN NUT STUCKING IN IMPELLAR , NUT WAS REMOVED AND IMPELLAR MADE FREE . PUMP TRIED PUT WORKING SATISFACTORY","2020-04-14","","Completed","2020-04-14","No","No","No","Internal"]
[null,null,null,null,14602,"46_29/04/2020 6:33:06 AM","2020-04-20","Defect","Ship Staff","Ship Staff Insp.","AE SW COOLING PUMP INLET PIPE STARTED LEAKING . ","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","PUMP STOPPED , COOLING WATER FOR AE SUPPLIED FROM FIRE AND GS PUMP LINE . PIPE REMOVED AND NEW PIPE FABRICATED . PIPE FITTED BACK ,PRESENTLY WORKING SATISFACTORY WITHOUT ANY LEAK .","2020-04-22","","Completed","2020-04-21","No","No","No","Internal"]
[null,null,null,null,14598,"46_09-Jun-20 4:34:05 PM","2020-05-01","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Working on pressure vessels permit not filled up for last Cargo hose test carried out on 22 Feb 2020.","Documentation","Cert. & Docu.","Inappropriate Procedure","","","","","The permit was filed in the appropriate file.","2020-05-31","","Completed","2020-05-06","No","No","No","Internal"]
[null,null,null,null,14599,"46_09-Jun-20 4:42:39 PM","2020-05-01","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","COT inspection records were not available last done Oct 2019 which was more than 6 months as per company policy","Documentation","Cert. & Docu.","Inappropriate Procedure","","","","","COT inspection record was done in feb filed in separate file.The COT inspection report filed in the appropriate file.","2020-05-31","","Completed","2020-05-06","No","No","No","Internal"]
[null,null,null,null,14600,"46_09-Jun-20 4:59:47 PM","2020-05-01","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Cargo Samples Landed on 06/01/2020 no receipt available.Cargo sample log to be kept updated ","Documentation","Cert. & Docu.","Human Error","","","","","The Sample landing receipt was filed in Sample log.Previously it was filed with Cargo papers.","2020-05-31","","Completed","2020-05-06","No","No","No","Internal"]
[null,null,null,null,14601,"46_09-Jun-20 5:06:52 PM","2020-05-01","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Lifting appliances records to be updated and all equipment to be tagged.","Documentation","Cert. & Docu.","Human Error","","","","","Lifting appliances records were updated.","2020-05-31","","Completed","2020-05-06","No","No","No","Internal"]
[null,null,null,null,14603,"46_09-Jun-20 5:09:44 PM","2020-05-01","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Tank cleaning records for last cleaning not updated checklist were incomplete.","Documentation","Cert. & Docu.","Human Error","","","","","The last Tank cleaning records were updated and filed.","2020-05-31","","Completed","2020-05-06","No","No","No","Internal"]
[null,null,null,null,14604,"46_09-Jun-20 5:14:59 PM","2020-05-01","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","MLC AUDIT:- Officer shower curtain torn and room not cleaned","Accommodation","General Appearance","Human Error","","","","","Shower curtain replaced with a new one and Shower room throughly cleaned.","2020-05-31","","Completed","2020-05-02","No","No","No","Internal"]
[null,null,null,null,14605,"46_09-Jun-20 5:18:04 PM","2020-05-01","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","MLC AUDIT :- All common spaces to have soap dispenser and Tissue rolls.","Accommodation","MLC Related","Human Error","","","","","Soap dispensers and tissue rolls kept at all common places.","2020-05-31","","Completed","2020-05-02","No","No","No","Internal"]
[null,null,null,null,14609,"46_15/05/2020 4:23:14 PM","2020-05-13","Defect","Ship Staff","Ship Staff Insp.","No.1 AC Compressor (STBD Side) is getting tripped after a run of approx 1 min run. When load change is there after run on unloaded condition trip is initiated.\n\nAfter start and running current for compressor No.1 checked and found above 35 Amps","Accommodation","Eng. / Strg. Comp.","Equipment Related","","","","","New AC compressor installed sucessfully and tried out. Working satisfactory.\n\nRunning condition current checked and found 16 Amps. Filter drier replaced with new one.\n\n","2020-05-15","","Completed","2020-05-15","No","No","No","Internal"]
[null,null,null,null,14606,"46_15/05/2020 4:30:08 PM","2020-05-14","Defect","Ship Staff","Ship Staff Insp.","Aft Hydraullic winch operating block oil leak from bottom side","Deck - Mooring Machinery","Mooring","Equipment Related","","","","","leaking and worn out plug repair carried out using 5 mm thick plate. Same O-ring used. Winch operated for 10 to 15 min. No leakages. All satisfactory.","2020-05-15","","Completed","2020-05-15","No","No","No","Internal"]
[null,null,null,null,14607,"46_12/6/2020 9:26:41 PM","2020-05-18","Observation","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","Torch equipment for testing of Flame detector was noted to be defective/\n\ndamaged","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","Requisition was raised and received new onboard","2020-05-19","","Completed","2020-05-19","No","No","No","External"]
[null,null,null,null,14608,"46_12/6/2020 9:32:38 PM","2020-05-18","Observation","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","Torch equipment for testing of Flame detector was noted to be defective/\n\ndamaged","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","Requisition was raised, recieved new onboard","2020-05-19","","Completed","2020-05-19","No","No","No","External"]
[null,null,null,null,14610,"46_12/6/2020 9:20:32 PM","2020-05-18","Observation","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","Cargo tank 3-Starboard Overfill alarm was noted to be functioning erratically, and\n\ngiving alarms frequently while the tank was at low level","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","REPLACED THE WHOLE UNIT","2020-06-30","","Completed","2020-06-09","No","No","No","External"]
[null,null,null,null,14615,"46_12/6/2020 9:36:27 PM","2020-05-18","Observation","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","Emergency Eye-wash and Shower near starboard manifold was found to be not in operational readiness, and\n\nfunctioning satisfactorily.","Deck - Pipe / Fittings","Emgcy. Systems","Equipment Related","","","","","Emergency eye wash replaced with new ","2020-05-26","","Completed","2020-05-24","No","No","No","External"]
[null,null,null,null,14587,"46_12/6/2020 8:53:34 PM","2020-05-18","Observation","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","Cargo Tank Cleaning Heater Steam Inlet Valve was noted to be leaking","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","","","",""," REPLACED IN DRYDOCK","2020-09-22","","Completed","2020-10-10","No","No","No","External"]
[null,null,null,null,14588,"46_14-Jun-20 9:30:25 AM","2020-05-18","Observation","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","There were isolated rust spots/patches observed on ship's hull.","Hull & Tanks","General Appearance","External Factors","","","","","Repair carried out in upcoming Drydock.","2020-09-22","","Completed","2020-10-12","No","No","No","External"]
[null,null,null,null,14611,"46_01/06/2020 7:58:51 AM","2020-05-22","Defect","Ship Staff","Ship Staff Insp.","Hydraulic oil lekage observed in cargo pump outlet pipe of 8p tank . on inspection found a pin hole in outlet pipe ","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","system was isolated . pipe remover and permanent repair carried out . pipe assemble back. system try out working satisfactory without any leaks  ","2020-05-23","","Completed","2020-05-23","No","No","No","Internal"]
[null,null,null,null,14612,"46_01/06/2020 8:05:06 AM","2020-05-23","Defect","Ship Staff","Ship Staff Insp.","small leak of lub oil from ae no 1 auto lub oil filter ","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","AE no 1 isolater , filter diassemble  and oil seal replaced with spare one . ae no 1 try out no leaks from filter obsereved","2020-05-24","","Completed","2020-05-24","No","No","No","Internal"]
[null,null,null,null,14613,"46_14-Jun-20 9:08:55 AM","2020-05-30","Observation","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","The upper temperature sensor in No. 4P cargo tank and low temperature sensor in No. 3P cargo tank found faulty ","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.23","Medium","","","Mussasino team attended faulty temperature sensors. 4P temperature PCP changed and under observation. ","2020-06-15","","Completed","2020-06-09","No","No","No","External"]
[null,null,null,null,14614,"46_14-Jun-20 9:39:20 AM","2020-05-30","Observation","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","Temporary repair was found on the compress air line on the main deck which was above No. 8S cargo tank ","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.7","High","","","Full length of deck air line replaced.","2020-06-30","","Completed","2020-06-12","No","No","No","External"]
[null,null,null,null,14616,"46_14-Jun-20 4:09:31 PM","2020-05-30","Defect","Ship Staff","Ship Staff Insp.","Leakage in  Ballast overboard line in  pump room.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","","","","","The damaged section dismantled from flange to flange, fabricated in work shop and fitted back. pressure test carried out/ Working satisfactorily.","2020-06-05","","Completed","2020-06-04","No","No","No","Internal"]
[null,null,null,null,14617,"46_12/7/2020 5:18:22 PM","2020-06-01","Defect","Ship Staff","Ship Staff Insp.","PORT SIDE PILOT LADDER FIRST STEP FOUND TWISTED.\t\t\t\t","Miscellaneous","Safety / LSA / FFA","Equipment Related","5.47","Low","","","NEW PILOT LADDER RECEIVED AND PUT IN USE.","2020-07-05","","Completed","2020-07-01","No","No","No","Internal"]
[null,null,null,null,14618,"46_20/06/2020 5:45:42 PM","2020-06-09","Defect","Ship Staff","Ship Staff Insp.","STP blower wear down in pulley and shaft due to which bearings worn out.","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","The temporary repairs has been carried out. Awaiting spares.","2020-07-07","","Completed","2020-07-03","No","No","No","Internal"]
[null,null,null,null,14619,"46_26/06/2020 7:05:22 AM","2020-06-21","Defect","Ship Staff","Ship Staff Insp.","OXYGEN ROOM PIPE TO ECR NEAR UNION GOT CORRODED.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","NEW PIPE TO BE FABRICATED.","2020-06-30",".","Completed","2020-06-24","No","No","No","Internal"]
[null,null,null,null,14620,"46_26/06/2020 7:16:13 AM","2020-06-21","Defect","Ship Staff","Ship Staff Insp.","REFER # 1 CONDENSOR COOLING WATER INLET , OUTLET AND BY PASS PIPE ARE LEAKING.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","NEEDS NEW PIPES TO BE FABRICTAED.","2020-07-15","","Completed","2020-07-03","No","No","No","Internal"]
[null,null,null,null,14621,"46_26/06/2020 7:19:00 AM","2020-06-22","Defect","Ship Staff","Ship Staff Insp.","EXHAUST GAS SOOT BLOWER WHEEL HANDLE BROKEN.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","WHEEL HANDLE TO BE FABRICATED.","2020-06-30","","Completed","2020-06-25","No","No","No","Internal"]
[null,null,null,null,14627,"46_26/06/2020 7:21:15 AM","2020-06-23","Defect","Ship Staff","Ship Staff Insp.","AUXILARY BOILER FORWARD GUAGE GLASS LEAKING.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","FORWARD GAUGE GLASS TO BE OVERHAULED.","2020-06-30","","Completed","2020-06-27","No","No","No","Internal"]
[null,null,null,null,14622,"46_26/06/2020 7:24:19 AM","2020-06-26","Defect","Ship Staff","Ship Staff Insp.","FRESH WATER GENERATOR OUTLET PIPE AFTER EDUCTOR LEAKING, HAVING SOFT PATCH.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","NEW PIPE NEED TO BE FABRICATED.","2020-06-30","","Completed","2020-06-27","No","No","No","Internal"]
[null,null,null,null,14623,"46_03/07/2020 7:37:34 AM","2020-06-26","Defect","Ship Staff","Ship Staff Insp.","AUXILARY ENGINE #1 TURNING GEAR INTERLOCK NOT WORKING.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","AWAITING SPARES. REQUISTION RAISED.","2020-07-10","","Completed","2020-07-02","No","No","No","Internal"]
[null,null,null,null,14624,"46_12/7/2020 4:48:40 PM","2020-06-26","Defect","Ship Staff","Ship Staff Insp.","AIR BRANCH LINE OF 6W, 7W & 9W FOUND CORRODED AND LEAKING.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","11.4","Very High","","","AIR BRANCH LINE REMOVED AND NEW LINE FABRICATED IN E/RM WORKSHOP AND FITTED IN PLACE.","2020-07-10","","Completed","2020-07-02","No","No","No","Internal"]
[null,null,null,null,14625,"46_12/7/2020 4:54:26 PM","2020-06-26","Defect","Ship Staff","Ship Staff Insp.","STEAM RETURN LINE SIGHTING TANK INLET & OUTLET PIPE LEAKING\t","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","11.4","Very High","","","STEAM RETURN LINE SIGHTING TANK REMOVED AND INLET/OUTLET PIPE FABRICATED IN WORKSHOP AND FITTED BACK IN PLACE.","2020-07-05","","Completed","2020-07-04","No","No","No","Internal"]
[null,null,null,null,14626,"46_04/07/2020 6:51:26 PM","2020-06-27","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","MAIN ENGINE CYLINDER OIL TRANSFER PUMP.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","NEW MAIN ENGINE CYLINDER OIL TRANSFER PUMP TO INSTALLED.","2020-07-08","","Completed","2020-07-04","No","No","No","Internal"]
[null,null,null,null,16860,"46_17/12/2020 4:00:50 PM","2020-06-28","Non Conformity","Ship Staff","Ship Staff Insp.","ISPS Visitors card 2 pcs missing (No. 2 & 6)","Documentation","ISPS Related","Knowledge Based","7.3","Low","","","All crew briefed on the best practices related to ISPS Visitors cards as per Fleet Memo - 004 of 2020","2020-08-10","","Completed","2020-06-30","No","No","No","Internal"]
[null,null,null,null,14628,"46_12/7/2020 5:25:51 PM","2020-06-29","Defect","Ship Staff","Ship Staff Insp.","FWD AND AFT MOORING WINCH LEVER LOCKING PIN FOUND BROKEN\t","Deck - Mooring Machinery","Mooring","Equipment Related","9.14","Medium","","","LOCKING PIN FABRICATED AND FIXED IN PLACE.","2020-07-15","","Completed","2020-07-11","No","No","No","Internal"]
[null,null,null,null,14629,"46_12/7/2020 5:10:33 PM","2020-07-02","Defect","Ship Staff","Ship Staff Insp.","Port manifold framo emergency stop box frame broken from the railing due to corroision\n\n\n\n","Cargo Mach.","Cargo / Ballast Systems","External Factors","8.1","Very High","","","New wooden frame made for framo emergency stop box and fixed on the railings.","2020-07-05","","Completed","2020-07-03","No","No","No","Internal"]
[null,null,null,null,14589,"46_16/7/2020 5:37:48 PM","2020-07-03","Defect","Ship Staff","Ship Staff Insp.","10 EEBD HOODS FOUND DAMAGED ON BOARD","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.44","High","","","EEBD HOOD REPLACED ON BOARD. ","2020-08-01","","Completed","2020-10-22","No","No","No","Internal"]
[null,null,null,null,14594,"46_04/07/2020 6:57:54 PM","2020-07-04","Defect","Ship Staff","Ship Staff Insp.","AUXILARY ENGINE #2 F.O TO D.O CHANGE OVER SWITCH MALFUNCTION.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","CHANGE THE F.O TO D.O CHANGE OVER SWITCH.","2020-07-15","","Completed","2020-07-15","No","No","No","Internal"]
[null,null,null,null,14630,"46_04/07/2020 7:03:40 PM","2020-07-04","Defect","Ship Staff","Ship Staff Insp.","AUXILARY ENGINE # 2 STARTING AIR REDUCER LEAKING.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","TO OVERHAUL AUXILARY ENGINE  STARTING AIR REDUCER.","2020-07-30","","Completed","2020-07-08","No","No","No","Internal"]
[null,null,null,null,14590,"46_11/07/2020 4:56:46 AM","2020-07-05","Defect","Ship Staff","Ship Staff Insp.","FRAMO OIL COOLER OUTLET  PIPE LINE HAVING SOFT PATCH.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","NEW PIPE LINE TO BE CROPPED AND FABRICATED.","2020-09-20","","Completed","2020-10-11","No","No","No","Internal"]
[null,null,null,null,14631,"46_11/07/2020 5:06:43 AM","2020-07-06","Defect","Ship Staff","Ship Staff Insp.","MAIN ENGINE CIRCULATING PUMP # 1 NOT DEVELOPING SUFFICENT PRESSURE","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","MAIN ENGINE CIRCULATING PUMP # 1 TO BE OVERHAULED.","2020-07-20","","Completed","2020-07-11","No","No","No","Internal"]
[null,null,null,null,14591,"46_11/07/2020 5:00:58 AM","2020-07-08","Defect","Ship Staff","Ship Staff Insp.","INCINERATOR PRIMARY FAN MOTOR, WASTE OIL PRESSURE SWITCH AND SOLENOID VALVE NOT WORKING.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","NEW PRIMARY FAN MOTOR TO BE INSTALLED ALONG WITH NEW PRESSURE SWITCH AND SOLENOID VALVE.","2020-08-15","","Completed","2020-09-18","No","No","No","Internal"]
[null,null,null,null,14592,"46_28/07/2020 7:36:00 PM","2020-07-09","Defect","Ship Staff","Ship Staff Insp.","ME SHAFT GROUNDING DEVICE NOT OPERATIONAL.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","THE RO HAS BEEN RAIESD. AWAITING SPARES. RO NO. WRUB200227","2020-08-30","","Completed","2020-11-17","No","No","No","Internal"]
[null,null,null,null,16861,"46_19/12/2020 5:03:11 PM","2020-07-09","Observation","Ship Staff","Nav Audit / Verification","EPIRB IMO SYMBOL AND MANUAL OPEARTION INSTRUCTION NOT POSTED","Navigation - Others","Navigation","Knowledge Based","4.25","Low","","","EPIRB IMO SYMBOL AND MUNAL OPEATING POSTED AT LOCATION. OFFICERS INFORMED TO TAKE MONTHLY ROUNDS TO INSPECT ALL IMO SYMBOLS ONBOARD AS PER PMS.","2020-07-30","","Completed","2020-07-10","No","No","No","Internal"]
[null,null,null,null,16862,"46_19/12/2020 5:09:27 PM","2020-07-09","Observation","Ship Staff","Nav Audit / Verification","FIRST AID KIT ON BRIDGE IMO SYSMBOL NOT POSTED","Miscellaneous","Safety / LSA / FFA","Knowledge Based","","","","","FIRST AID IMO SYMBOL POSTED AT LOCATION. OFFICERS INFORMED TO TAKE MONTHLY ROUNDS TO INSPECT ALL IMO SYMBOLS ONBOARD.","2020-07-30","","Completed","2020-07-10","No","No","No","Internal"]
[null,null,null,null,16863,"46_19/12/2020 5:13:36 PM","2020-07-09","Observation","Ship Staff","Nav Audit / Verification","HARD COPY OF SHIPBOARD EMERGENCY PLAN ON BRIDGE OF OLD EDITION","Documentation","Cert. & Docu.","Behaviour Based","","","","","NEW REVISION SEP PLACED ON THE BRIDGE. ALL OFFICERS TO BE GIVEN A COPY OF HSQEE REVISIONS LIST MONTHLY AND CARRY OUT CHANGES AS REQUIRED.","2020-07-30","","Completed","2020-07-12","No","No","No","Internal"]
[null,null,null,null,16864,"46_19/12/2020 5:23:20 PM","2020-07-09","Non Conformity","Ship Staff","Nav Audit / Verification","AIS TRANSMITTING WRONG MMSI NUMBER","Navigation - DGPS / EPFS / AIS","Navigation","Human Error","4.7","High","","","VESSEL INFORMED OFFICE AND RECEIVED INSTRUCTIONS FROM MAKERS OF PROCEDURE TO CHANGE MMSI ON TH AIS. ALL OFFICERS INFORMED AS PER DEPARTURE CHECKLIST TO CHECK OWNSHIP & VOAYGE DATA ON AIS.","2020-07-30","","Completed","2020-07-09","No","No","No","Internal"]
[null,null,null,null,16865,"46_19/12/2020 5:27:08 PM","2020-07-09","Observation","Ship Staff","Nav Audit / Verification","WHISTLEBLOWER POLICY FOR SHIPBOARD PERSONNEL NOT POSTED IN COMMON AREAS.","Documentation","Cert. & Docu.","Knowledge Based","","","","","WHISTLW BLOWER POLICY FOR SHIPBOARD PERSONNEL POSTED IN COMMON AREAS. ALL CREW TO BE MADE FAMILIAR WITH COMPANY POLICIES DURING JOIING IN FAMILIARIZATION CHECK LIST.","2020-07-30","","Completed","2020-07-10","No","No","No","Internal"]
[null,null,null,null,16866,"46_19/12/2020 5:30:00 PM","2020-07-09","Observation","Ship Staff","Nav Audit / Verification","WORK PLACE DISCRIMINATION POLICY NOT POSTED AND CREW NOT FAMILIAR","Documentation","Cert. & Docu.","Knowledge Based","","","","","WORKPLACE DISCRIMINATION POLICY POSTED AND ALL CREW MADE FAMILIAR DURING SAFETY MEETING","2020-07-30","","Completed","2020-07-10","No","No","No","Internal"]
[null,null,null,null,14593,"46_13/07/2020 7:31:06 PM","2020-07-11","Defect","Ship Staff","Ship Staff Insp.","AUXILARY ENGINE # 3 FLYWHEEL GEAR TEETH WORN OUT FOR STARTING AIR MOTOR.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","THE NEW GEAR TEETH TO PUT ON FLYWHEEL.","2020-09-30","","Completed","2020-10-13","No","No","No","Internal"]
[null,null,null,null,14633,"46_19/07/2020 7:28:38 AM","2020-07-11","Defect","Ship Staff","Ship Staff Insp.","BOILER WATER CIRCULATING PUMP # 1 GAVE ABNORMAL SOUND AND CONTINOUS WATER WAS COMMING FROM GLAND EVEN AFTER TIGHTENING FULL GLAND COVER. FOUND GLAND PACKING BOX ERRODED DUE TO WHICH GLAND GOT BURNT.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","BOILER WATER CIRCULATING PUMP # 1 NEEDS TO BE OVERHAULED AND PACKING BOX ALONG WITH SLEEVE AND GLANDS NEEDS TO BE RENEWED.","2020-07-20","","Completed","2020-07-12","No","No","No","Internal"]
[null,null,null,null,14632,"46_12/7/2020 5:34:29 PM","2020-07-12","Defect","Ship Staff","Ship Staff Insp.","7S CARGO TANK PRESSURE SENSOR SHOWING \"ERROR 4\" , SHOWING TANK PRESSURE 50 - 60 KPa.\t","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.13","Low","","","PRESSOR SENSOR CHECKED, REMOVED, CLEANED AND LOCAL TEST OF PRESSURE SENSOR CARRIED OUT. ALL FOUND IN ORDER. 7S TANK SHOWING CORRECT PRESSURE WITHOUT ANY ALARM/ERROR.","2020-07-20","","Completed","2020-07-14","No","No","No","Internal"]
[null,null,null,null,14634,"46_19/07/2020 7:16:24 AM","2020-07-12","Defect","Ship Staff","Ship Staff Insp.","ENGINE STEAM SERVICE LINE VALVE LEAKING.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","STEAM SERVICE LINE VALVE TO BE RENEWED.","2020-07-25","","Completed","2020-07-19","No","No","No","Internal"]
[null,null,null,null,14635,"46_2/8/2020 6:05:58 PM","2020-07-26","Observation","Ship Staff","Ship Staff Insp.","8p cargo tank framo pump pressure gauge found in-operational/ defective ","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.18","Low","","","8P framo pump pressure gauge changed with spare pressure gauge.","2020-07-30","","Completed","2020-07-29","No","No","No","Internal"]
[null,null,null,null,16867,"46_17/12/2020 3:28:25 PM","2020-07-26","Non Conformity","Ship Staff","Ship Staff Insp.","8P cargo tank framo pump local pressure gauge found not working/defective during pre-arrival check & test.","Cargo Mach.","Cargo / Ballast Systems","Knowledge Based","8.23","Medium","","","Replaced defective pressure gauge with spare onboard and tested found working in order.","2020-07-30","","Completed","2020-07-29","No","No","No","Internal"]
[null,null,null,null,15631,"46_28/11/2020 4:23:23 PM","2020-07-29","Defect","Ship Staff","Ship Staff Insp.","LOW SEA CHEST PURGING COCK NOT FITTED.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","LOW SEA CHEST PURGING COCK NEEDS TO BE FABRICATED.","2020-08-30","","Completed","2020-08-02","No","No","No","Internal"]
[null,null,null,null,15038,"46_04/08/2020 7:44:31 AM","2020-07-29","Defect","Ship Staff","Ship Staff Insp.","LOW SEA CHEST PURGING COCK NOT FITTED.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","LOW SEA CHEST PURGING COCK NEEDS TO BE FABRICATED.","2020-08-10","","Completed","2020-08-02","No","No","No","Internal"]
[null,null,null,null,15632,"46_28/11/2020 4:24:54 PM","2020-07-30","Defect","Ship Staff","Ship Staff Insp.","HIGH SEA CHEST PURGING COCK NOT FITTED.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","HIGH SEA CHEST PURGING COCK NEEDS TO BE FABRICATED.","2020-08-30","","Completed","2020-08-03","No","No","No","Internal"]
[null,null,null,null,15039,"46_04/08/2020 7:46:56 AM","2020-07-30","Defect","Ship Staff","Ship Staff Insp.","HIGH SEA CHEST PURGING COCK NOT FITTED.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","HIGH SEA CHEST PURGING COCK NEEDS TO BE FABRICATED.","2020-08-10","","Completed","2020-08-03","No","No","No","Internal"]
[null,null,null,null,15633,"46_28/11/2020 4:26:47 PM","2020-08-02","Defect","Ship Staff","Ship Staff Insp.","STEAM TRACING LINE NEAR MAIN ENGINE INLET VALVE LEAKING.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","STEAM TRACING LINE NEAR MAIN ENGINE INLET VALE NEEDS TO BE FABRICATED WITH ARMATO COUPLING.","2020-08-30","","Completed","2020-08-08","No","No","No","Internal"]
[null,null,null,null,15040,"46_09/08/2020 6:31:09 PM","2020-08-02","Defect","Ship Staff","Ship Staff Insp.","STEAM TRACING LINE NEAR MAIN ENGINE INLET VALVE LEAKING.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","THE LEAKING STEAM TRACING LINE NEEDS TO BE CROPPED AND FITTED WITH NEW ARAMOTO COUPLING.","2020-08-10","","Completed","2020-08-08","No","No","No","Internal"]
[null,null,null,null,15634,"46_28/11/2020 4:28:39 PM","2020-08-03","Defect","Ship Staff","Ship Staff Insp.","ME JACKET WATER OUTLET TEMPERATURE SENSOR(THERMOSTAT) NOT OPERATIONAL.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","ME JACKET WATER OUTLET TEMPERATURE SENSOR(THERMOSTAT) NEEDS TO BE CHANGED WITH NEW ONE.","2020-08-30","","Completed","2020-10-13","No","No","No","Internal"]
[null,null,null,null,15041,"46_21/08/2020 4:49:58 AM","2020-08-03","Defect","Ship Staff","Ship Staff Insp.","ME JACKET WATER OUTLET TEMPERATURE SENSOR(THERMOSTAT) NOT OPERATIONAL.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","THE REQUESTION HAS BEEN RAISED AWAITING SPARES. R.O WRUB200234.","2020-09-30","","Completed","2020-10-13","No","No","No","Internal"]
[null,null,null,null,15635,"46_28/11/2020 4:31:39 PM","2020-08-04","Defect","Ship Staff","Ship Staff Insp.","OWS OUTLET LINE NEAR SAFETY VALVE HAVING SOFT PATCH.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","NEW OWS OUTLET LINE NEAR SAFETY VALVE NEEDS TO BE FABRICATED.","2020-08-30","","Completed","2020-08-09","No","No","No","Internal"]
[null,null,null,null,15042,"46_09/08/2020 6:32:59 PM","2020-08-04","Defect","Ship Staff","Ship Staff Insp.","OWS OUTLET LINE NEAR SAFETY VALVE HAVING SOFT PATCH.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","NEW PIPE LINE NEEDS TO BE FABRICATED.","2020-08-12","","Completed","2020-08-09","No","No","No","Internal"]
[null,null,null,null,15636,"46_28/11/2020 4:33:50 PM","2020-08-05","Defect","Ship Staff","Ship Staff Insp.","EMERGENCY GENERATOR STAND BY LIGHT INDICATION ON EMERGENCY CONTROL  AND ECR PANNEL NOT SHOWING STBY INDICATION.","Critical Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","EMERGENCY GENERATOR STAND BY LIGHT INDICATION ON EMERGENCY CONTROL  AND ECR PANNEL FAULT TO BE RECTIFIED.","2020-10-30","","Completed","2020-10-03","No","No","No","Internal"]
[null,null,null,null,15043,"46_23/08/2020 6:04:09 PM","2020-08-05","Critical Equipment","Ship Staff","Ship Staff Insp.","EMERGENCY GENERATOR STAND BY LIGHT INDICATION ON EMERGENCY CONTROL  AND ECR PANNEL NOT SHOWING STBY INDICATION.","Critical Equip.","Emgcy. Systems","Equipment Related","10.32","Very High","","","TROUBLE SHOOTING TO BE CARRIED OUT FOR STBY LIGHT INDICATION ON EMERGENCY AND ECR CONTROL PANNEL.","2020-09-30","","Completed","2020-10-03","No","No","No","Internal"]
[null,null,null,null,16868,"46_17/12/2020 3:17:29 PM","2020-08-05","Observation","Ship Staff","Ship Staff Insp.","During cargo tank cleaning operation observed 3 tank cleaning machine (2TC machine of 10S & 1 TC Machine of 10P) not working","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","Tank Cleaning machine overhauled and rectified.","2020-08-20","","Completed","2020-08-18","No","No","No","Internal"]
[null,null,null,null,15637,"46_28/11/2020 4:35:20 PM","2020-08-06","Defect","Ship Staff","Ship Staff Insp.","HFO# 2 PURIFIER WATER REDUCER LEAKING FROM DIAPHGRAM AND SECURING PIN HOLDING REDUCER BROKEN.","E/R - Purifier","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","HFO# 2 PURIFIER WATER REDUCER LEAKING FROM DIAPHGRAM AND SECURING PIN HOLDING REDUCER NEEDS TO BE FABRICATED.","2020-08-30","","Completed","2020-08-15","No","No","No","Internal"]
[null,null,null,null,15044,"46_21/08/2020 5:15:42 AM","2020-08-06","Defect","Ship Staff","Ship Staff Insp.","HFO# 2 PURIFIER WATER REDUCER LEAKING FROM DIAPHGRAM AND SECURING PIN HOLDING REDUCER BROKEN.","E/R - Purifier","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","HFO# 2 PURIFIER WATER REDUCER TO OVERHAUL AND SECURING PIN TO BE FABRICATED.","2020-08-20","","Completed","2020-08-15","No","No","No","Internal"]
[null,null,null,null,15638,"46_28/11/2020 4:36:38 PM","2020-08-08","Defect","Ship Staff","Ship Staff Insp.","AUXILARY ENGINE # 3 UNIT #3 INDICATOR COCK LEAKING.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","AUXILARY ENGINE # 3 UNIT #3 INDICATOR COCK TO BE CHANGED WITH OVERHAULED ONE.","2020-08-30","","Completed","2020-08-19","No","No","No","Internal"]
[null,null,null,null,15639,"46_28/11/2020 4:38:11 PM","2020-08-08","Defect","Ship Staff","Ship Staff Insp.","AUXILARY ENGINE # 3 ACB OFF LIGHT INDICATION ON MSB NOT INDICATING WHILE GENERATOR IS STARTED AND OFF LOADED.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","AUXILARY ENGINE # 3 ACB OFF LIGHT INDICATION ON MSB NOT INDICATING WHILE GENERATOR IS STARTED AND OFF LOADED. THE FAULT TO BE RECTIFIED.","2020-10-30","","Completed","2020-10-03","No","No","No","Internal"]
[null,null,null,null,15045,"46_21/08/2020 5:03:56 AM","2020-08-08","Defect","Ship Staff","Ship Staff Insp.","AUXILARY ENGINE # 3 UNIT #3 INDICATOR COCK LEAKING.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","AUXILARY ENGINE # 3 UNIT #3 INDICATOR COCK NEEDS TO BE REPLACED WITH OVERHAULED ONE.","2020-08-20","","Completed","2020-08-19","No","No","No","Internal"]
[null,null,null,null,15046,"46_23/08/2020 6:17:52 PM","2020-08-08","Defect","Ship Staff","Ship Staff Insp.","AUXILARY ENGINE # 3 ACB OFF LIGHT INDICATION ON MSB NOT INDICATING WHILE GENERATOR IS STARTED AND OFF LOADED.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","TROUBLE SHOOTING FOR THE ACB OFF LIGHT INDICATION ON MSB TO CARRY OUT.","2020-09-30","","Completed","2020-10-03","No","No","No","Internal"]
[null,null,null,null,15640,"46_28/11/2020 4:39:28 PM","2020-08-10","Defect","Ship Staff","Ship Staff Insp.","BOILER FEED WATER CONTROLER BY PASS VALVE NOT HOLDING/ LEAKING.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","BOILER FEED WATER CONTROLER BY PASS VALVE TO BE OVERHAULED.","2020-09-30","","Completed","2020-08-13","No","No","No","Internal"]
[null,null,null,null,15047,"46_21/08/2020 4:57:11 AM","2020-08-10","Defect","Ship Staff","Ship Staff Insp.","BOILER FEED WATER CONTROLER BY PASS VALVE NOT HOLDING/ LEAKING.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","BOILER FEED WATER CONTROLLER BYPASS VALVE NEEDS TO BE OVERHUALED/ CHANGED DEPENDING UPON CONDITION OF VALVE.","2020-08-20","","Completed","2020-08-13","No","No","No","Internal"]
[null,null,null,null,15641,"46_28/11/2020 4:41:06 PM","2020-08-14","Defect","Ship Staff","Ship Staff Insp.","HOT WATER CIRCULATING PUMP MECHINICAL SEAL LEAKING. ","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","HOT WATER CIRCULATING PUMP NEEDS TO BE OVERHAULED. ","2020-08-30","","Completed","2020-08-28","No","No","No","Internal"]
[null,null,null,null,15048,"46_29/08/2020 7:33:06 PM","2020-08-14","Defect","Ship Staff","Ship Staff Insp.","HOT WATER CIRCULATING PUMP MECHINICAL SEAL LEAKING. ","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","THE HOT WATER CIRCULATING PUMP NEEDS TO BE OVERHAULED. ","2020-08-30","","Completed","2020-08-28","No","No","No","Internal"]
[null,null,null,null,15642,"46_28/11/2020 4:43:07 PM","2020-08-17","Defect","Ship Staff","Ship Staff Insp.","STEAM TRACING LINE LEAKING ABOVE AE # 2 AIR DUCT.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","STEAM TRACING LINE LEAKING ABOVE AE # 2 AIR DUCT NEEDS TO BE FABRICATED WITH ARMATO COUPLING.","2020-09-30","","Completed","2020-08-26","No","No","No","Internal"]
[null,null,null,null,15049,"46_29/08/2020 7:35:50 PM","2020-08-17","Defect","Ship Staff","Ship Staff Insp.","STEAM TRACING LINE LEAKING ABOVE AE # 2 AIR DUCT.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","THE STEAM TRACING LINE NEEDS TO BE CROPPED UP AND FITTED WITH NEW ARAMOTO COUPLING.","2020-08-30","","Completed","2020-08-26","No","No","No","Internal"]
[null,null,null,null,15643,"46_28/11/2020 4:45:54 PM","2020-08-20","Defect","Ship Staff","Ship Staff Insp.","AE PORT SIDE JACKET WATER COOLER  INLET PIPE  LEAKING NEAR THE FLANGE.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","AE PORT SIDE JACKET WATER COOLER  INLET PIPE TO BE WELDED NEAR THE FLANGE. IF REQUIRED CROP AND RENEW THE PIPE FROM THE FLANGE AREA.","2020-09-30","","Completed","2020-08-29","No","No","No","Internal"]
[null,null,null,null,15050,"46_29/08/2020 7:49:45 PM","2020-08-20","Defect","Ship Staff","Ship Staff Insp.","AE PORT SIDE JACKET WATER COOLER  INLET PIPE  LEAKING NEAR THE FLANGE.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","AE PORT SIDE JACKET WATER COOLER INLET PIPE GASKET TO BE RENEWED / WELDING TO BE CARRIED OUT AT THE FLANGE INLET SEAM.","2020-08-30","","Completed","2020-08-29","No","No","No","Internal"]
[null,null,null,null,15644,"46_28/11/2020 4:47:14 PM","2020-08-22","Defect","Ship Staff","Ship Staff Insp.","INCINERATOR WASTE OIL TANK QUICK CLOSING VALVE LEAKING WHEN IN CLOSE POSITION.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","INCINERATOR WASTE OIL TANK QUICK CLOSING VALVE NEEDS TO BE OVERHAULED.","2020-08-30","","Completed","2020-09-08","No","No","No","Internal"]
[null,null,null,null,15051,"46_17/09/2020 11:11:29 AM","2020-08-22","Defect","Ship Staff","Ship Staff Insp.","INCINERATOR WASTE OIL TANK QUICK CLOSING VALVE LEAKING WHEN IN CLOSE POSITION.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","INCINERATOR WASTE OIL TANK QUICK CLOSING VALVE TO BE OVERHAULED. VALVE AND VALVE SEAT TO BE LAPPED AND AIR PISTON O RINGS TO BE CHANGED.","2020-09-30","","Completed","2020-09-08","No","No","No","Internal"]
[null,null,null,null,15645,"46_28/11/2020 4:49:18 PM","2020-08-28","Defect","Ship Staff","Ship Staff Insp.","SEWAGE 3 WAY CHANGE OVER VALVE AND NON RETURN FLAP VALVE IS STUCK IN ONE POSITION.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","SEWAGE 3 WAY CHANGE OVER VALVE AND NON RETURN FLAP VALVE TO BE OVERHAULED AS ITS STUCK IN ONE POSITION.","2020-09-29","","Completed","2020-09-10","No","No","No","Internal"]
[null,null,null,null,5176,"38_25/10/2019 7:12:24 PM","2020-08-28","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Several U Clamps for cargo and hydraulic lines on the Main Deck are rusted. Same to be de rusted and painted.","Hull & Tanks","General Appearance","External Factors","11.5","Medium","","","All branch pipes completed. Started with main Pipes. Plan to complete by 31 Jan 2019","2021-01-30","","Completed","2020-12-29","No","No","No","Internal","Pls revert with progress update for said job."]
[null,null,null,null,15052,"46_17/09/2020 11:16:31 AM","2020-08-28","Defect","Ship Staff","Ship Staff Insp.","SEWAGE 3 WAY CHANGE OVER VALVE AND NON RETURN FLAP VALVE TO BE OVERHAULED AS ITS STUCK IN ONE POSITION.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","SEWAGE 3 WAY CHANGE OVER VALVE AND NRV FLAP VALVE TO BE OVERHAULED.","2020-09-20","","Completed","2020-09-10","No","No","No","Internal"]
[null,null,null,null,15646,"46_28/11/2020 4:50:57 PM","2020-09-01","Defect","Ship Staff","Ship Staff Insp.","SEWAGE DISCHAGRE PUMP MACHINICAL SEAL LEAKING. ","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","SEWAGE DISCHAGRE PUMP NEEDS TO BE OVERHAULED.","2020-09-30","","Completed","2020-09-11","No","No","No","Internal"]
[null,null,null,null,15647,"46_28/11/2020 4:52:24 PM","2020-09-01","Defect","Ship Staff","Ship Staff Insp.","SEWAGE PUMP DISCHARGE PIPE HAVING SOFT PATCH / LEAKING NEAR ELBOW.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","SEWAGE PUMP DISCHARGE PIPE NEEDS TO BE FABRICATED.","2020-09-30","","Completed","2020-09-11","No","No","No","Internal"]
[null,null,null,null,15653,"46_28/11/2020 6:29:58 PM","2020-09-01","Defect","Ship Staff","Ship Staff Insp.","THE MAIN ENGINE FLOW METER NOT OPERATIONAL.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","THE MAIN ENGINE FLOW METER NEEDS TO BE REPLACED WITH NEW ONE.","2020-12-30","","Completed","2020-11-30","No","No","No","Internal"]
[null,null,null,null,15029,"46_15/11/2020 7:22:55 PM","2020-09-01","Defect","Ship Staff","Ship Staff Insp.","THE MAIN ENGINE FLOW METER NOT OPERATIONAL.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","THE NEW FLOWMETER NEEDS TO BE INSTALLED. THE REQUESTION HAS BEEN RAISED WRUB200251. ONCE RECIEVED WILL REPLACE THE SAME.","2020-12-30","","Completed","2020-11-30","No","No","No","Internal"]
[null,null,null,null,15053,"46_17/09/2020 11:23:51 AM","2020-09-01","Defect","Ship Staff","Ship Staff Insp.","SEWAGE DISCHAGRE PUMP MACHINICAL SEAL LEAKING. ","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","SEWAGE DISCHARGE PUMP MACHINICAL SEAL TO BE CHANGED AND PUMP TO BE OVERHAULED.","2020-09-25","","Completed","2020-09-11","No","No","No","Internal"]
[null,null,null,null,15062,"46_17/09/2020 11:32:01 AM","2020-09-01","Defect","Ship Staff","Ship Staff Insp.","SEWAGE PUMP DISCHARGE PIPE HAVING SOFT PATCH / LEAKING NEAR ELBOW.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","NEW SEWAGE PUMP DISCHARGE PIPE TO BE FABRICATED.","2020-09-30","","Completed","2020-09-11","No","No","No","Internal"]
[null,null,null,null,15648,"46_28/11/2020 4:54:24 PM","2020-09-02","Defect","Ship Staff","Ship Staff Insp.","BOW THRUSTER TELEMOTOR COUPLING BETWEEN PUMP AND MOTOR BROKEN / MISSING.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","BOW THRUSTER TELEMOTOR COUPLING BETWEEN PUMP AND MOTOR NEEDS TO BE FABRICATED.","2020-09-30","","Completed","2020-09-09","No","No","No","Internal"]
[null,null,null,null,15054,"46_17/09/2020 11:29:30 AM","2020-09-02","Defect","Ship Staff","Ship Staff Insp.","BOW THRUSTER TELEMOTOR COUPLING BETWEEN PUMP AND MOTOR BROKEN / MISSING.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","BOW THRUSTER TELEMOTOR COUPLING TO BE FABRICATED.","2020-09-02","","Completed","2020-09-09","No","No","No","Internal"]
[null,null,null,null,15649,"46_28/11/2020 4:56:51 PM","2020-09-20","Defect","Ship Staff","Ship Staff Insp.","CONTROL AIR DRYER NOT OPERATIONAL.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","NEW CONTROL AIR DRYER TO BE INSTALLED.","2020-10-30","","Completed","2020-10-14","No","No","No","Internal"]
[null,null,null,null,15055,"46_15/11/2020 6:38:52 PM","2020-09-20","Defect","Ship Staff","Ship Staff Insp.","CONTROL AIR DRYER NOT OPERATIONAL.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","THE NEW CONTROL AIR DRYER TO BE INSTALLED ALONG WITH THE AIR LINE MODIFICATIONS.","2020-10-20","","Completed","2020-10-14","No","No","No","Internal"]
[null,null,null,null,15650,"46_28/11/2020 4:58:39 PM","2020-09-21","Defect","Ship Staff","Ship Staff Insp.","THE FEED FILTER TANK HIGH LEVEL FLOAT TO BE INSTALLED AND FLANGE MODICATION TO BE DONE.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","THE FEED FILTER TANK HIGH LEVEL FLOAT TO BE INSTALLED AND FLANGE MODICATION TO BE DONE. ","2020-10-30","","Completed","2020-10-15","No","No","No","Internal"]
[null,null,null,null,15056,"46_15/11/2020 6:41:59 PM","2020-09-21","Defect","Ship Staff","Ship Staff Insp.","THE FEED FILTER TANK HIGH LEVEL FLOAT TO BE INSTALLED AND FLANGE MODICATION TO BE DONE.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","THE FLOAT HAS BEEN ORDERED ONCE RECIEVED WILL BE INSTALLING THE SAME.","2020-10-20","","Completed","2020-10-15","No","No","No","Internal"]
[null,null,null,null,16869,"46_17/12/2020 3:02:31 PM","2020-09-22","Non Conformity","Ship Staff","Ship Staff Insp.","Not using leading light for checking Gyro error","Navigation - Others","Navigation","Knowledge Based","4.9","Medium","","","Training given to all deck officer and cadet how to check gyro error using leading light.","2020-10-01","","Completed","2020-09-22","No","No","No","Internal"]
[null,null,null,null,15651,"46_28/11/2020 5:00:20 PM","2020-09-23","Defect","Ship Staff","Ship Staff Insp.","THE DRINKING WATER PIPE LINE HAS PIN HOLE NEAR THE FLANGE","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","THE DRINKING WATER PIPE LINE NEEDS TO BE FABRICATED.","2020-09-23","","Completed","2020-10-10","No","No","No","Internal"]
[null,null,null,null,15057,"46_15/11/2020 6:44:38 PM","2020-09-23","Defect","Ship Staff","Ship Staff Insp.","THE DRINKING WATER PIPE LINE HAS PIN HOLE NEAR THE FLANGE.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","THE DRINKING WATER PUMP TO BE STOPPED AND ALL VALVES TO SHUT. THE LINE TO BE REMOVED AND NEW LINE TO BE FABRICATED.","2020-10-20","","Completed","2020-10-10","No","No","No","Internal"]
[null,null,null,null,15652,"46_28/11/2020 5:01:50 PM","2020-09-25","Defect","Ship Staff","Ship Staff Insp.","THE HOT WATER RECIRCULATING LINE HAS SOFT PATCH.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","THE NEW HOT WATER RECIRCULATING LINE NEEDS TO BE FABRICATED.","2020-10-30","","Completed","2020-10-01","No","No","No","Internal"]
[null,null,null,null,15058,"46_15/11/2020 6:46:54 PM","2020-09-25","Defect","Ship Staff","Ship Staff Insp.","THE HOT WATER RECIRCULATING LINE HAS SOFT PATCH.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","THE NEW LINE TO BE FABRICATED. ALL THE MATERIALS ON BOARD.","2020-10-20","","Completed","2020-10-01","No","No","No","Internal"]
[null,null,null,null,15192,"46_24/11/2020 2:23:39 PM","2020-09-28","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","No.3 DG LO cooler to ohaul & leaking gasket to replace with new. \n\n","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","no # 3 l.o cooler gasket to be replcaed with owners supplied gaskets","2020-10-30","","Completed","2020-10-15","No","No","No","Internal"]
[null,null,null,null,15059,"46_17/11/2020 6:53:47 AM","2020-09-28","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","AE# 3 LUBE OIL COOLER OIL LEAKING FROM GASKET.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","THE AE# 3 LUBE OIL COOLER TO BE OPEN UP CLEANED AND GASKET TO BE RENEWED.","2020-10-30","","Completed","2020-10-15","No","No","No","Internal"]
[null,null,null,null,15060,"46_17/11/2020 7:00:41 AM","2020-09-28","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","THE GMDSS BATTERY TO BE REPLACED.","Navigation - GMDSS & Communication","Navigation","Equipment Related","","","","","THE EXSISTING BATTERY  TO BE REPLACED BY NEW SUPPLIED BATTERY FOR GMDSS.","2020-10-30","","Completed","2020-10-28","No","No","No","Internal"]
[null,null,null,null,15061,"46_17/11/2020 7:05:13 AM","2020-09-28","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","AE # 3 TURBOCHARGER TO BE PROTECTED FROM ANY SPRAY OF MAIN ENGINE.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","THE GUARD TO BE FABRICATED FOR SPLASH PROTECTION IN FRONT OF AE # 3 TURBOCHARGER.","2020-10-30","","Completed","2020-10-29","No","No","No","Internal"]
[null,null,null,null,15063,"46_17/11/2020 7:10:42 AM","2020-09-28","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ALL THE POSTERS TO BE REMOVED FROM ENGINE CONTROL ROOM.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","THE ECR BULKHEAD TO BE CLEANED AND ALL POSTERS TO BE PUT ON GREEN BOARD.","2020-11-30","","Completed","2020-11-12","No","No","No","Internal"]
[null,null,null,null,15064,"46_17/11/2020 4:06:25 PM","2020-09-28","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ALL THE THREE GENERATOR TURBOCHARGER LAGGING IN BAD CONDITION.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","THE ALL THREE GENERATOR TURBOCHARGER LAGGING TO BE REPLACED WITH OWNERS SUPPLIED LAGGINGS.","2020-11-30","","Completed","2020-11-13","No","No","No","Internal"]
[null,null,null,null,15065,"46_17/11/2020 4:18:23 PM","2020-09-28","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ALL BOILER MOUNTING LAGGING TO BE REPLACED/RENEW.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","THE ALL BOILER LAGGING TO BE RENEWED BY OWNERS SUPPLIED LAGGINGS.","2020-10-30","","Completed","2020-10-30","No","No","No","Internal"]
[null,null,null,null,15066,"46_17/11/2020 4:23:11 PM","2020-09-28","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","BOILER PRESSURE GAUGE CONNECTION LINE HAS PIN HOLE.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","THE NEW BOILER GAUGE CONNECTION LINE TO BE FABRICATED.","2020-11-30","","Completed","2020-11-02","No","No","No","Internal"]
[null,null,null,null,15067,"46_17/11/2020 4:26:11 PM","2020-09-28","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","THE AE# 3 LUBE OIL PRESSURE GAUGE DEFECTIVE.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","THE NEW AE# 3 LUBE OIL PRESSURE GAUGE TO BE INSTALLED.","2020-10-30","","Completed","2020-10-15","No","No","No","Internal"]
[null,null,null,null,15068,"46_17/11/2020 4:30:26 PM","2020-09-28","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","THE EMERGENCY FIRE PUMP SUCTION LINE LAGGING TO REPLACE/RENEW.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","THE LAGGING TO BE RENEWED BY OWNERS SUPPLIED LAGGING.","2020-10-30","","Completed","2020-10-28","No","No","No","Internal"]
[null,null,null,null,15069,"46_17/11/2020 4:35:28 PM","2020-09-28","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ENGINE ROOM STORES TO BE PROPERLY ARRANGED.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","ALL THE SPARES TO BE SEGRIGATED AND STORE ROOM TO BE PROPERLY ARRANGED.","2020-11-30","","Completed","2020-11-05","No","No","No","Internal"]
[null,null,null,null,15070,"46_17/11/2020 4:46:04 PM","2020-09-28","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","THE MAINE ENGINE HIGH PRESSURE PIPE LAGGING TO RENEW/ REPLACE.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","THE ALL HIGH PRESSURE PIPE ON MAIN ENGINE LAGGING TO RENEW BY OWNERS SUPPLIED LAGGINGS.","2020-10-30","","Completed","2020-10-29","No","No","No","Internal"]
[null,null,null,null,15071,"46_17/11/2020 4:52:24 PM","2020-09-28","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","LIFE BOAT BATTERY PERMANENT CHARGING ARRANGMENT TO MAKE.","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","THE LIFE BOAT BATTERY PERMANENT CHARGING ARRANGMENT TO MODIFY WITH OWNERS SUPPLIED SPARES.","2020-11-30","","Completed","2020-11-08","No","No","No","Internal"]
[null,null,null,null,15080,"46_17/11/2020 4:49:31 PM","2020-09-28","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","AE# 1 STARTING AIR MOTOR DISTANCE TO FLYWHEEL GEAR TEETH TO CHECK.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","THE FLYWHEEL GEAR TEETH DISTANCE FROM STARTING AIR MOTOR TO CHECK AND IF REQUIRED ADJUST BETWEEN 6.6 TO 9.0 MM","2020-10-30","","Completed","2020-10-26","No","No","No","Internal"]
[null,null,null,null,16870,"46_17/12/2020 2:54:43 PM","2020-10-10","Non Conformity","Ship Staff","Ship Staff Insp.","GMDSS Batteries fitted of incorrect specification ","Navigation - GMDSS & Communication","Communication","Knowledge Based","4.23","High","","","New Batteries of 200A  were ordered in Dry dock and replaced after receipt.","2020-11-01","","Completed","2020-10-30","No","No","No","Internal"]
[null,null,null,null,15030,"46_17/11/2020 6:49:11 AM","2020-10-15","Defect","Ship Staff","Ship Staff Insp.","AE# 1 FLYWHEEL GEAR TEETH FOR STARTING AIR MOTOR WORN OUT.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","THE NEW FLY WHEEL GEAR TEETH TO BE INSTALLED IN FUTURE. (BUT FOR THE EXSISTING TEETH GRINDING TO BE CARRIED OUT).VESSEL HAS NO OPERATIONAL ISSUE","2021-01-30","","Completed","2020-11-07","No","No","No","Internal","NOTED VESSEL HAS NO OPERATIONAL ISSUE"]
[null,null,null,null,15081,"46_16-Nov-20 10:53:38 AM","2020-10-15","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","GMDSS batteries to be replaced","Navigation - GMDSS & Communication","Communication","Equipment Related","4.21","High","","","New Batteries fitted and charged.","2020-10-30","","Completed","2020-10-28","No","No","No","Internal"]
[null,null,null,null,15188,"46_24/11/2020 3:23:24 PM","2020-10-16","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Accommodation Doors hydraulic locks to adjust","Miscellaneous","General Appearance","Equipment Related","","","","","all hydraulic locks to be adjusted. ","2020-11-30","","Completed","2020-11-22","No","No","No","Internal"]
[null,null,null,null,15072,"46_16-Nov-20 11:31:36 AM","2020-10-16","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Steel works carried out at 2P and 7ws WBT to painted 2nd coat.","Hull & Tanks","Cargo / Ballast Systems","Equipment Related","11.11","Very High","","","2nd coat paint  applied at ballast tanks.","2020-11-06","","Completed","2020-11-04","No","No","No","Internal"]
[null,null,null,null,15189,"46_24/11/2020 2:21:42 PM","2020-10-17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Make sure old DG Lube oil filters are disposed to avoid confusion. The filters are added in critical spare art list (3 sets) as min spares. Same to be also updated in CE & 2E handover notes","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","The filters are added in critical spare art list (3 sets) as min spares. Same to be also updated in CE & 2E handover notes","2020-10-30","","Completed","2020-10-20","No","No","No","Internal"]
[null,null,null,null,15190,"46_24/11/2020 2:26:02 PM","2020-10-17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Boiler chemical dosing & nitrates dosing in jacket system to be carried out & brought to normal levels.\n\n     \n\n","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","theboiler water treatment chemicals and jacket water chemicals to be added to bring to normal levels.","2020-10-30","","Completed","2020-10-21","No","No","No","Internal"]
[null,null,null,null,15191,"46_24/11/2020 2:27:53 PM","2020-10-17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","New supplied GMDSS & General batteries to be fitted & charged.\n\n","Navigation - GMDSS & Communication","Navigation","Equipment Related","","","","","the gmdss battery to be changed","2020-11-30","","Completed","2020-10-28","No","No","No","Internal"]
[null,null,null,null,15193,"46_24/11/2020 2:31:46 PM","2020-10-17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Splash protection to be made in front of AE 3 turbocharger to protect any spray from the main engine.\n\n\n\n","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","the splash protection board to be fabricated","2020-11-30","","Completed","2020-11-05","No","No","No","Internal"]
[null,null,null,null,15194,"46_24/11/2020 2:36:48 PM","2020-10-17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","There plenty thermometer and gauges not working, broken during repairs. Same to be replaced & Ro to be raised as required.","Critical Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","all the defective thermometer and pressure guages to be replaced with new one.","2020-11-30","","Completed","2020-11-26","No","No","No","Internal"]
[null,null,null,null,15195,"46_24/11/2020 2:43:13 PM","2020-10-17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Engine Control room all bulkheads to be soap washed Posters to be removed and put on a green board in engine room, order for green board.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","bulkhead to be cleaned and green board to be installed","2020-11-30","","Completed","2020-11-12","No","No","No","Internal"]
[null,null,null,null,15196,"46_24/11/2020 2:47:31 PM","2020-10-17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Insulation for boiler valves to be fitted back.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","all insulation to be made and changed with owners supplied blankets","2020-11-30","","Completed","2020-10-30","No","No","No","Internal"]
[null,null,null,null,15197,"46_24/11/2020 2:38:30 PM","2020-10-17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ME Turbocharger air filters diff manometer missing, same to fix & carry out body cleaning.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","the missing diff manometer to be fixed","2020-11-30","","Completed","2020-11-05","No","No","No","Internal"]
[null,null,null,null,15198,"46_24/11/2020 2:34:14 PM","2020-10-17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Engine room to be properly cleaned from TOP to bottom Soap wash.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","engine room house keeping to be carried out properly","2020-11-30","","Completed","2020-11-24","No","No","No","Internal"]
[null,null,null,null,15199,"46_24/11/2020 2:49:28 PM","2020-10-17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Leak at boiler vent valve to be rectified at anchorage.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","vent valve leak to be rectified","2020-11-30","","Completed","2020-11-02","No","No","No","Internal"]
[null,null,null,null,15200,"46_24/11/2020 2:53:33 PM","2020-10-17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","All DG Engine cylinder heads & entablature to be cleaned & Painted.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","all dg engine cylinder head to be cleaned and painted.","2020-11-30","","Completed","2020-11-22","No","No","No","Internal"]
[null,null,null,null,15201,"46_24/11/2020 2:55:45 PM","2020-10-17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Insulation near Emg. escape exit to be renewed as falling off","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","insulation on emg escape to be renewed.","2020-11-30","","Completed","2020-11-25","No","No","No","Internal"]
[null,null,null,null,15202,"46_24/11/2020 2:45:33 PM","2020-10-17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","New Turbocharger blankets to be made, arranged from shore, same to be fitted once received.","E/R - Aux. Engine,E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","new turbocharger blanket to be changed with owners supplied blanket","2020-11-20","","Completed","2020-11-13","No","No","No","Internal"]
[null,null,null,null,15203,"46_24/11/2020 2:59:28 PM","2020-10-17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Main air Compressors pumping out too much oil, adjust the feed rate as per maker recommendation","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","main air compressor to be overhauled","2020-11-30","","Completed","2020-11-04","No","No","No","Internal"]
[null,null,null,null,15204,"46_24/11/2020 2:51:36 PM","2020-10-17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","AE3 LO press gauge defective, recheck on it, Same to be renewed.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","the defective lo pressure guage to be renewed.","2020-11-30","","Completed","2020-10-19","No","No","No","Internal"]
[null,null,null,null,15205,"46_24/11/2020 3:02:09 PM","2020-10-17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","All minor oil leaks in the engine room to be rectified.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","minor leaks to be rectified and stopped.","2020-10-30","","Completed","2020-11-26","No","No","No","Internal"]
[null,null,null,null,15206,"46_24/11/2020 3:07:40 PM","2020-10-17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","PMS inventory not updated at many equipment’s in PAL PMS ","Documentation","Eng. / Strg. Comp.","Equipment Related","","","","","pms inventory to be updates in pal","2020-11-30","","Completed","2020-11-27","No","No","No","Internal"]
[null,null,null,null,15207,"46_24/11/2020 2:41:02 PM","2020-10-17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Bilges & floor top full of oil to be cleaned and washed.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","bilges to be cleaned and painted","2020-11-30","","Completed","2020-11-21","No","No","No","Internal"]
[null,null,null,null,15208,"46_24/11/2020 3:16:55 PM","2020-10-17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Accommodation cleaning to carry out & plan for painting white colour to get more luminance, CCR bulkheads to be cleaned","Accommodation","Eng. / Strg. Comp.","Equipment Related","11.13","Low","","","Accomodation inside bulkheads painted white.","2020-11-30","","Completed","2020-12-23","No","No","No","Internal"]
[null,null,null,null,15209,"46_24/11/2020 3:09:54 PM","2020-10-17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","All broken chairs in ECR to dispose off & replace with new provided","Accommodation","Eng. / Strg. Comp.","Equipment Related","","","","","all engine room broken chair to be replaced with owners supplied ones.","2020-11-30","","Completed","2020-11-09","No","No","No","Internal"]
[null,null,null,null,15210,"46_24/11/2020 3:25:58 PM","2020-10-17","Observation","Ship Staff","Ship Staff Insp.","All company policy posters to be removed from the walls and to be put on a green board in accommodation","Documentation","General Appearance","Equipment Related","","","","","all company policy psoters to be put on green board.","2020-11-30","","Completed","2020-11-22","No","No","No","Internal"]
[null,null,null,null,15211,"46_24/11/2020 3:19:50 PM","2020-10-17","Observation","Ship Staff","Ship Staff Insp.","Check FWG distillate pump spares, order if required as per operational spares.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","pump spares to check and order","2020-11-30","","Completed","2020-11-13","No","No","No","Internal"]
[null,null,null,null,15212,"46_24/11/2020 3:28:25 PM","2020-10-17","Observation","Ship Staff","Ship Staff Insp.","All the plate type coolers on board, always min 50% of gaskets should be present on board.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","all gasket inventry to be taken and if less then 50% rqf to be made","2020-11-30","","Completed","2020-12-25","No","No","No","Internal"]
[null,null,null,null,15214,"46_24/11/2020 3:04:13 PM","2020-10-17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Vessel to be supplied with a queue machine & Ultra sonic cleaner, Raise RFQ","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","ultra sonic cleaner and queue machine to be ordered.","2020-11-30","","Completed","2020-12-25","No","No","No","Internal"]
[null,null,null,null,15215,"46_24/11/2020 3:06:01 PM","2020-10-17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Engine room Stores to organised and spares to be arranged as per mentioned box","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","engine room stores to organise and arrange","2020-11-30","","Completed","2020-11-14","No","No","No","Internal"]
[null,null,null,null,15216,"46_24/11/2020 3:37:26 PM","2020-10-17","Defect","Ship Staff","Ship Staff Insp.","Lagging to be fitted on newly fabricated steam line, except the expansion bellow.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","lagging to be fitted on steam line","2020-11-30","","Completed","2020-11-20","No","No","No","Internal"]
[null,null,null,null,15217,"46_24/11/2020 3:40:16 PM","2020-10-17","Defect","Ship Staff","Ship Staff Insp.","Forecastle mesh to be power tooled & painted.","Deck - Pipe / Fittings","General Appearance","Equipment Related","8.49","Medium","","","forecastle mesh  renewed.","2020-11-30","","Completed","2020-11-23","No","No","No","Internal"]
[null,null,null,null,15218,"46_24/11/2020 3:42:33 PM","2020-10-17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Remaining Hull anodes on deck to be kept in forecastle.","Hull & Tanks","General Appearance","Equipment Related","","","","","hull anodes  kept on forecastle deck.","2020-11-29","","Completed","2020-11-01","No","No","No","Internal"]
[null,null,null,null,15219,"46_24/11/2020 3:44:52 PM","2020-10-17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","FN tape to be applied on ME Fuel High pressure pipe.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","high pressure fuel oil to be put with anti splash tape","2020-11-30","","Completed","2020-10-29","No","No","No","Internal"]
[null,null,null,null,15220,"46_24/11/2020 3:47:21 PM","2020-10-17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ER skylight hatch cover to paint, rubber gasket to be applied.","Deck - Pipe / Fittings","General Appearance","Equipment Related","","","","","Engine room skylight hatch painted and gasket  changed.","2020-11-30","","Completed","2020-11-03","No","No","No","Internal"]
[null,null,null,null,15221,"46_24/11/2020 3:49:22 PM","2020-10-17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Port side aft winch motor pressure pipe to replace with new fabricated pipe.","Deck - Mooring Machinery","Mooring","Equipment Related","","","","","Port side aft winch motor pressure pipe to replace with new fabricated pipe.","2020-11-30","","Completed","2020-11-04","No","No","No","Internal"]
[null,null,null,null,15222,"46_24/11/2020 3:50:41 PM","2020-10-17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Stbd side aft winch motor inlet v/v handle broken, same to be renewed with new.","Deck - Mooring Machinery","Mooring","Equipment Related","","","","","Stbd side aft winch motor inlet v/v handle, renewed with new.","2020-11-30","","Completed","2020-10-22","No","No","No","Internal"]
[null,null,null,null,15223,"46_24/11/2020 3:54:36 PM","2020-10-17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Lifeboat battery arrangement to fix for permanent charging with spares supplied.","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","Lifeboat battery arrangement fixed for permanent charging with owners supplied spares.","2020-11-30","","Completed","2020-11-08","No","No","No","Internal"]
[null,null,null,null,15224,"46_24/11/2020 3:58:15 PM","2020-10-17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Hot work permit to be applied complete remaining deck fitting jobs like 4P support angle bar for FW line, LB embarkation deck plating renewal etc.","Documentation","General Appearance","Equipment Related","","","","","hot work permit applied for  L/B embarkation deck plating renewal and filed.","2020-11-30","","Completed","2020-10-22","No","No","No","Internal"]
[null,null,null,null,15225,"46_24/11/2020 3:34:46 PM","2020-10-17","Observation","Ship Staff","Ship Staff Insp.","FW line & tracing steam to be tested for any leaks & then Lagging to be fitted in remaining area.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","fw line and tracing steam line to be tested after fitting","2020-11-30","","Completed","2020-11-07","No","No","No","Internal"]
[null,null,null,null,15226,"46_24/11/2020 4:02:48 PM","2020-10-17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Ballast tanks 2P, 7 P & S where steel work has been carried out, 2nd coat to be applied on painted areas.","Hull & Tanks","Structural Condn. / WT integrity ","Equipment Related","","","","","second coat  applied on 2p, 7p & s ballast tanks.","2020-11-30","","Completed","2020-11-04","No","No","No","Internal"]
[null,null,null,null,15227,"46_24/11/2020 4:04:39 PM","2020-10-17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Detailed PMS reporting to be done for major jobs carried out in DD related to PMS (Planned or unplanned) with spare parts consumed, service report attached etc.","Documentation","Eng. / Strg. Comp.","Equipment Related","","","","","all dd jobs to be reported on pal, with job description, pictures and service report attached.","2020-11-30","","Completed","2020-12-07","No","No","No","Internal"]
[null,null,null,null,15228,"46_24/11/2020 3:53:02 PM","2020-10-17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","AE1 flywheel cover to be takeout & gear to check for any indent, same to be polished as required. distance of air motor to be adjusted from 9 mm to 6.6 mm","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","AE1 flywheel gear teeth to be polished as required. distance of air motor to be adjusted from 9 mm to 6.6 mm","2020-11-29","","Completed","2020-12-22","No","No","No","Internal"]
[null,null,null,null,15229,"46_24/11/2020 4:00:24 PM","2020-10-17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ME performance to be taken at different RPMs both loaded & ballast condition to keep as reference","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","me performance to be taken on loaded and ballast condition.","2020-11-30","","Completed","2020-11-02","No","No","No","Internal"]
[null,null,null,null,15032,"46_08-Nov-20 10:22:23 AM","2020-10-17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Deck Air pipeline fabricated sections provided by yard to be renewed & Valves to be fitted accordingly","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","","","","","ALL FABRICATED SECTION DERUSTED & 1ST / 2ND PRIMER APPLIED. SECTION TO RENEW IN NEXT BALLAST PASSAGE","2021-01-31","","Completed","2021-02-28","No","No","No","Internal","plan to complete at earliest"]
[null,null,null,null,15073,"46_08-Nov-20 9:57:57 AM","2020-10-17","Observation","Ship Staff","Suptd. Insp.","All broken chairs in ECR to dispose off & replace with new provided","Accommodation","General Appearance","Equipment Related","","","","","ALL BROKEN CHAIRS REPLACED WITH NEW","2020-10-24","","Completed","2020-10-26","Yes","No","No","Internal"]
[null,null,null,null,15074,"46_08-Nov-20 10:04:00 AM","2020-10-17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Accommodation Doors hydraulic locks to adjust","Accommodation","General Appearance","Equipment Related","","","","","ALL DOORS HYDRAULIC LOCKS ADJUSTED","2020-10-24","","Completed","2020-11-05","Yes","No","No","Internal"]
[null,null,null,null,15075,"46_08-Nov-20 10:26:12 AM","2020-10-17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","FW line & tracing steam to be tested for any leaks & then Lagging to be fitted in remaining area.","Deck - Pipe / Fittings","General Appearance","Equipment Related","","","","","FW LINE & STEAM TRACING LINE TESTED. LAGGING FITTED.","2020-11-07","","Completed","2020-11-05","Yes","No","No","Internal"]
[null,null,null,null,15076,"46_08-Nov-20 10:29:21 AM","2020-10-17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Lagging to be fitted on newly fabricated steam line, except the expansion bellow.","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.5","Medium","","","LAGGING FITTED ON NEWLY FABRICATED STEAM LINE.","2020-11-17","","Completed","2020-11-03","Yes","No","No","Internal"]
[null,null,null,null,15077,"46_08-Nov-20 10:32:48 AM","2020-10-17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Forecastle mesh to be power tooled & painted.\n\n     \n\n","Deck - Pipe / Fittings","General Appearance","External Factors","11.3","Medium","","","FORECASTLE STORE VET MESH DERUSTED & PAINTED.","2020-11-07","","Completed","2020-11-02","Yes","No","No","Internal"]
[null,null,null,null,15078,"46_08-Nov-20 10:14:18 AM","2020-10-17","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","All company policy posters to be removed from the walls and to be put on a green board in accommodation","Documentation","Cert. & Docu.","Behaviour Based,Human Error,Inappropriate Procedure","","","","","GREEN BOARD RFQ RAISED, AWAITING ORDER","2020-11-07","","Completed","2020-11-16","Yes","No","No","Internal"]
[null,null,null,null,15079,"46_17/11/2020 12:04:11 PM","2020-10-17","Defect","Ship Staff","Ship Staff Insp.","Lifeboat embarkation deck plating renewal.","LSA / FFA","Safety / LSA / FFA","Equipment Related","11.4","Very High","","","Lifeboat embarkation deck plating renewed.","2020-11-16","","Completed","2020-10-22","No","No","No","Internal"]
[null,null,null,null,15628,"46_28/11/2020 6:35:53 PM","2020-10-18","Defect","Ship Staff","Ship Staff Insp.","PORT SIDE STEERING GEAR OIL LEAKING FROM HYDRAULIC PUMP OIL SEAL.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","PORT SIDE STEERING GEAR OIL SEAL TO BE REPLACED.","2020-12-30","","Completed","2020-12-25","No","No","No","Internal"]
[null,null,null,null,15629,"46_28/11/2020 6:37:16 PM","2020-10-18","Defect","Ship Staff","Ship Staff Insp.","STBD SIDE STEERING GEAR OIL LEAKING FROM HYDRAULIC PUMP OIL SEAL.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","STBD SIDE STEERING GEAR OIL SEAL NEEDS TO BE REPLACED.","2020-12-30","","Completed","2020-12-25","No","No","No","Internal"]
[null,null,null,null,15035,"46_17/11/2020 6:38:02 AM","2020-10-18","Defect","Ship Staff","Ship Staff Insp.","PORT SIDE STEERING GEAR OIL LEAKING FROM HYDRAULIC PUMP OIL SEAL.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","THE PORT SIDE STEERING GEAR HYDRUALIC PUMP OIL SEAL TO BE RENEWED.","2020-12-30","","Completed","2020-12-25","No","No","No","Internal"]
[null,null,null,null,15036,"46_17/11/2020 6:42:51 AM","2020-10-18","Defect","Ship Staff","Ship Staff Insp.","STBD SIDE STEERING GEAR OIL LEAKING FROM HYDRAULIC PUMP OIL SEAL.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","THE STBD SIDE STEERING GEAR OIL LEAKING FROM HYDRAULIC PUMP OIL SEAL TO BE RENEWED.","2020-12-30","","Completed","2020-12-25","No","No","No","Internal"]
[null,null,null,null,15654,"46_28/11/2020 5:29:40 PM","2020-10-20","Defect","Ship Staff","Ship Staff Insp.","BILGE LINE NEAR AFT BILGE WELL HAVING SOFT PATCH AND PIN HOLE.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","THE NEW LINE NEEDS TO BE FABRICATED.","2020-10-30","","Completed","2020-11-13","No","No","No","Internal"]
[null,null,null,null,15655,"46_28/11/2020 5:31:41 PM","2020-10-20","Defect","Ship Staff","Ship Staff Insp.","THE SLUDGE PUMP IS NOT BUILDING SUFFICIENT PRESSURE.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","THE SLUDGE PUMP TO BE OVERHAULED.","2020-10-30","","Completed","2020-10-22","No","No","No","Internal"]
[null,null,null,null,15656,"46_28/11/2020 5:33:42 PM","2020-10-20","Defect","Ship Staff","Ship Staff Insp.","THE ME LUBE OIL PURIFER GAVE ABNORMAL SOUND AND VIBRATION DURING DESLUDING.","E/R - Purifier","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","THE ME LUBE OIL PURIFER NEEDS TO BE OVERHAULED. ALL THE VERTICAL AND HORIZONTAL SHAFT BEARING NEEDS TO BE REPLACED WITH NEW ONE.","2020-10-30","","Completed","2020-10-23","No","No","No","Internal"]
[null,null,null,null,15082,"46_15/11/2020 6:59:20 PM","2020-10-20","Defect","Ship Staff","Ship Staff Insp.","BILGE LINE NEAR AFT BILGE WELL HAVING SOFT PATCH AND PIN HOLE.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","THE NEW BILGE LINE NEEDS TO BE FABRICATED.","2020-11-30","","Completed","2020-11-13","No","No","No","Internal"]
[null,null,null,null,15083,"46_15/11/2020 7:19:30 PM","2020-10-20","Defect","Ship Staff","Ship Staff Insp.","THE SLUDGE PUMP IS NOT BUILDING SUFFICIENT PRESSURE.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","THE SLUDGE PUMP NEEDS TO BE OVERHAULED. IF REQUIRED THE STATOR NEEDS TO BE REPLACED. ","2020-10-30","","Completed","2020-10-22","No","No","No","Internal"]
[null,null,null,null,15084,"46_16/11/2020 6:05:17 AM","2020-10-20","Breakdown","Ship Staff","Ship Staff Insp.","THE ME LUBE OIL PURIFER GAVE ABNORMAL SOUND AND VIBRATION DURING DESLUDING.","E/R - Purifier","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","THE MAIN ENGINE LUBE OIL PURIFER NEEDS TO BE OVERHAULED. IF REQUIRED CHANGE THE BEARINGS AND BOWL CLEANING TO BE CARRIED OUT.","2020-10-30","","Completed","2020-10-23","No","No","No","Internal"]
[null,null,null,null,15657,"46_28/11/2020 5:35:47 PM","2020-10-21","Defect","Ship Staff","Ship Staff Insp.","THE MAIN ENGINE LUBE OIL CONTROLLER MALFUNCTIONING","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","THE MAIN ENGINE LUBE OIL CONTROLLER CALIBRATION TO BE CARRIED OUT.","2020-11-30","","Completed","2020-11-09","No","No","No","Internal"]
[null,null,null,null,16871,"46_19/12/2020 5:14:09 AM","2020-10-21","Defect","Ship Staff","Ship Staff Insp.","ME FUEL PUMP LINKAGES TO BE CHANGED FOR ALL UNITS.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","THE REQUESTION HAS BEEN MADE ONCE RECIEVED WILL REPLACE THE SAME. THE RQF WRUB 200304","2020-12-30","","Completed","2020-12-03","No","No","No","Internal"]
[null,null,null,null,15085,"46_15/11/2020 7:03:33 PM","2020-10-21","Defect","Ship Staff","Ship Staff Insp.","THE MAIN ENGINE LUBE OIL CONTROLLER MALFUNCTIONING.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","THE MAIN ENGINE LUBE OIL CONTROLLER NEEDS TO BE CALIBRATED.","2020-11-15","","Completed","2020-11-09","No","No","No","Internal"]
[null,null,null,null,16872,"46_19/12/2020 5:19:50 AM","2020-10-22","Defect","Ship Staff","Ship Staff Insp.","ME REVERSING CYLINDER TO CHANGE. AS PER MARICO REPORT.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","ME REVERSING CYLINDER TO REPLACE AND REQUESTION HAS BEEN MADE THE REQUESTION NO IS WRUB 200308. ONCE RECIEVE WILL REPLACE THE SAME.","2020-12-30","","Completed","2020-12-08","No","No","No","Internal"]
[null,null,null,null,15658,"46_28/11/2020 5:37:06 PM","2020-10-24","Defect","Ship Staff","Ship Staff Insp.","THE MAIN ENGINE VISCOTHERM MAFFUNCTIONING ON VLSFO.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","THE MAIN ENGINE VISCOTHERM NEEDS TO BE CALIBRATED.","2020-11-30","","Completed","2020-11-09","No","No","No","Internal"]
[null,null,null,null,15086,"46_15/11/2020 7:11:08 PM","2020-10-24","Defect","Ship Staff","Ship Staff Insp.","THE MAIN ENGINE VISCOTHERM MAFFUNCTIONING ON VLSFO.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","THE MAIN ENGINE VISCOTHERM NEED TO BE CALIBATED ON BOTH LSMGO AS WELL AS VLSFO.","2020-11-15","","Completed","2020-11-09","No","No","No","Internal"]
[null,null,null,null,15659,"46_28/11/2020 5:39:09 PM","2020-10-29","Defect","Ship Staff","Ship Staff Insp.","MAINE ENGINE UNIT # 4 FUEL INJECTOR LEAKING.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","MAINE ENGINE UNIT # 4 FUEL INJECTOR NEEDS TO BE REPLACED WITH OVERHAULED ONE.","2020-11-30","","Completed","2020-11-12","No","No","No","Internal"]
[null,null,null,null,15087,"46_15/11/2020 7:26:14 PM","2020-10-29","Defect","Ship Staff","Ship Staff Insp.","MAINE ENGINE UNIT # 4 FUEL INJECTOR LEAKING.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","THE MAIN ENGINE UNIT #4 FUEL INJECTOR NEEDS TO BE REPLACED WITH OVERHAULED ONE.","2020-11-15","","Completed","2020-11-12","No","No","No","Internal"]
[null,null,null,null,15660,"46_28/11/2020 5:40:50 PM","2020-11-08","Defect","Ship Staff","Ship Staff Insp.","THE FRESH WATER GENERATOR SUCTION PIPE HAVING PIN HOLE NEAR THE ELBOW.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","THE FRESH WATER GENERATOR NEW SUCTION PIPE NEEDS TO BE FABRICATED.","2020-11-30","","Completed","2020-11-11","No","No","No","Internal"]
[null,null,null,null,15088,"46_15/11/2020 7:32:12 PM","2020-11-08","Defect","Ship Staff","Ship Staff Insp.","THE FRESH WATER GENERATOR SUCTION PIPE HAVING PIN HOLE NEAR THE ELBOW.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","THE  NEW SUCTION PIPE LINE NEEDS TO BE FABRICATED.","2020-11-30","","Completed","2020-11-11","No","No","No","Internal"]
[null,null,null,null,15661,"46_28/11/2020 5:43:20 PM","2020-11-09","Defect","Ship Staff","Ship Staff Insp.","THE MAIN AIR COMPRESSOR # 1 GAVE ABNORMAL SOUND AND ITS AMPERE STARTED HUNTING.","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","THE MAIN AIR COMPRESSOR # 1 NEEDS TO BE OVERHAULED.","2020-11-30","","Completed","2020-11-12","No","No","No","Internal"]
[null,null,null,null,15090,"46_17-Nov-20 10:44:20 AM","2020-11-11","Defect","Ship Staff","Ship Staff Insp.","Local display units of 2P,3P and 7P COT not showing any parameters.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.13","Low","","","Rectified the connection problem in one and replaced the display unit in two others.","2020-11-18","","Completed","2020-11-16","No","No","No","Internal"]
[null,null,null,null,15662,"46_28/11/2020 5:46:21 PM","2020-11-12","Defect","Ship Staff","Ship Staff Insp.","THE MAIN ENGINE JACKET WATER INLET PIPE LINE HAVING SOFT PATCH AND HAS PIN HOLE NEAR THE FLANGE.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","THE MAIN ENGINE JACKET WATER NEW INLET PIPE LINE NEEDS TO BE FABRICATED.","2020-11-30","","Completed","2020-11-17","No","No","No","Internal"]
[null,null,null,null,15091,"46_15/11/2020 7:28:57 PM","2020-11-12","Defect","Ship Staff","Ship Staff Insp.","THE MAIN ENGINE JACKET WATER INLET PIPE LINE HAVING SOFT PATCH AND HAS PIN HOLE NEAR THE FLANGE.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","THE NEW PIPE LINE NEEDS TO BE FABRICATED.","2020-11-30","","Completed","2020-11-17","No","No","No","Internal"]
[null,null,null,null,15663,"46_28/11/2020 5:49:21 PM","2020-11-13","Defect","Ship Staff","Ship Staff Insp.","FRESH WATER GENERATOR DISCHARGE PIPE HAVING PIN HOLE AND SOFT PATCH.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","THE NEW FRESH WATER GENERATOR DISCHARGE PIPE NEEDS TO BE FABRICATED.","2020-11-30","","Completed","2020-11-15","No","No","No","Internal"]
[null,null,null,null,15095,"46_15/11/2020 6:56:33 PM","2020-11-13","Defect","Ship Staff","Ship Staff Insp.","FRESH WATER GENERATOR DISCHARGE PIPE HAVING PIN HOLE AND SOFT PATCH.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","THE NEW DISCHARGE PIPE NEEDS TO BE FABRICATED.","2020-11-30","","Completed","2020-11-15","No","No","No","Internal"]
[null,null,null,null,15664,"46_28/11/2020 5:50:59 PM","2020-11-14","Defect","Ship Staff","Ship Staff Insp.","FRAMO INLET PIPE TO THE COOLER HAVING PIN HOLE NEAR THE FLANGE.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","FRAMO INLET PIPE TO THE COOLER TO BE FABRICATED.","2020-11-30","","Completed","2020-11-17","No","No","No","Internal"]
[null,null,null,null,15092,"46_17-Nov-20 10:27:52 AM","2020-11-14","Defect","Ship Staff","Ship Staff Insp.","PORTSIDE LIFEBOAT FWD BLOCK SWIVEL WAS NOT MOVING AND FREEZED AT PLACE.","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.29","High","","","FWD SWIVEL OF PORTSIDE LIFEBOAT REPAIRED AND NOW WORKING SATISFACTORILY. ","2020-11-16","","Completed","2020-11-16","No","No","No","Internal"]
[null,null,null,null,15093,"46_15/11/2020 7:36:24 PM","2020-11-14","Defect","Ship Staff","Ship Staff Insp.","FRAMO INLET PIPE TO THE COOLER HAVING PIN HOLE NEAR THE FLANGE.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","THE PIPE LINE NEEDS TO CROPPED NEAR THE FLANGE AND NEW PIPE WITH FALNGE TO  BE FABRICATED.","2020-11-30","","Completed","2020-11-17","No","No","No","Internal"]
[null,null,null,null,15665,"46_28/11/2020 5:52:30 PM","2020-11-15","Defect","Ship Staff","Ship Staff Insp.","THE ECR AC COOLING WATER OUTLET PIPE HAS PIN HOLE NEAR THE OUTLET FLANGE.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","THE ECR AC COOLING WATER OUTLET PIPE NEEDS TO BE FABRICATED.","2020-11-30","","Completed","2020-11-17","No","No","No","Internal"]
[null,null,null,null,15094,"46_16/11/2020 6:14:37 AM","2020-11-15","Defect","Ship Staff","Ship Staff Insp.","THE ECR AC COOLING WATER OUTLET PIPE HAS PIN HOLE NEAR THE OUTLET FLANGE.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","THE NEW COOLING WATER OUTLET PIPE NEEDS TO BE FABRICATED.","2020-11-30","","Completed","2020-11-17","No","No","No","Internal"]
[null,null,null,null,16880,"46_19/12/2020 5:10:14 AM","2020-11-17","Defect","Ship Staff","Ship Staff Insp.","SERVICE TANK STEAM OUTLET VALVE LEAKING FROM VALVE BONET","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","SERVICE TANK STEAM OUTLET VALVE TO BE OVERHAULED / REPLACED WITH NEW ONE.","2020-12-30","","Completed","2020-12-01","No","No","No","Internal"]
[null,null,null,null,16881,"46_17/12/2020 2:37:32 PM","2020-11-21","Non Conformity","Ship Staff","Ship Staff Insp.","Aft poop deck fire hydrant found leaking","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.38","High","","","Replaced spare hydrant onboard","2020-11-30","","Completed","2020-11-30","No","No","No","Internal"]
[null,null,null,null,16873,"46_17/12/2020 2:46:57 PM","2020-11-23","Non Conformity","Ship Staff","Ship Staff Insp.","Pumproom port side bilge alarm found not working during routine test","Miscellaneous","MARPOL Related","Equipment Related","6.11","High","","","The bilge larm unit dismantled, cleaned, repaired, derusted and fitted back, tested and found operational. ","2020-12-30","","Completed","2020-11-30","No","No","No","Internal"]
[null,null,null,null,16874,"46_19/12/2020 4:39:53 PM","2020-11-23","Observation","Ship Staff","Nav Audit / Verification","VHF No. 1 Illumination Light out of Order.","Navigation - GMDSS & Communication","Navigation","Equipment Related","","","","","Raised Requisition. All OOW are advised all faulty/out of order equipments to immediately address and create RO immediately if needed","2020-11-30","WRUB200330","Completed","2020-11-30","No","No","No","Internal"]
[null,null,null,null,16875,"46_19/12/2020 4:48:01 PM","2020-11-23","Observation","Ship Staff","Nav Audit / Verification","APPENDIX 11 - Ship specific ECDIS alarm Managment still not made as the office sample provided still not found in PAL and 12.02.34.035- Record of Non WGS ENC form same still not found in PAL but Temporary Ship List made in Passage Plan.","Documentation","Cert. & Docu.","Behaviour Based","","","","","Asked to HSQE to provide the office sample of Ship Specific ECDIS alarm Management and 12.01.34.035 Record of Non WGS ENC form. Advised to all OOW not to hesitate to call master attention if in doubt or required office attention or clarification via master.","2020-12-31","","Completed","2020-12-01","No","No","No","Internal"]
[null,null,null,null,16876,"46_19/12/2020 4:57:23 PM","2020-11-23","Observation","Ship Staff","Nav Audit / Verification","No. 1 ECDIS UPS Battery expired since April 2020","Navigation - ECDIS","Navigation","Equipment Related","","","","","Raised RO. All OOWs are advised all units/parts/battery/UPS with expiration, 3 months before the expiration to bring to master attention and create RO as required.","2020-11-30","WRUB2000332","Completed","2020-11-30","No","No","No","Internal"]
[null,null,null,null,16883,"46_19/12/2020 4:32:58 PM","2020-11-23","Non Conformity","Ship Staff","Nav Audit / Verification","Activation of BNWAS 1st, 2nd & 3rd stage alarm not carried out weekly same not recorded in deck log book but carry out as per PMS 3monthly","Navigation - VDR / BNWAS","Navigation","Knowledge Based","4.1","High","","","Advised person in-charged to carry out the test weekly in accordance of company QDMS and recorded in deck log book onward. All officers advised to cross check the frequency of test and records of other equipments in accordance of company QDMS.","2020-12-31","","Completed","2020-11-30","No","No","No","Internal"]
[null,null,null,null,16877,"46_17/12/2020 2:15:40 PM","2020-11-27","Observation","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","The Face shield & googles in the paint store were dirty & ages, these face shield and googles were replaced before inspector disembarkation.","Miscellaneous","Safety / LSA / FFA","Human Error","5.5","Low","","","Immediately replaced with new spare onboard. Training carried out to all crew.","2020-11-30","","Completed","2020-11-30","No","No","No","External"]
[null,null,null,null,16878,"46_17/12/2020 2:24:38 PM","2020-11-27","Observation","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","Turning up a line on poop bitt was to take one full turn instead of two full turns around the leading post before belaying figure of eights. This findings was rectified when pointed out by the inspector.","Miscellaneous","Mooring","Knowledge Based","9.9","Medium","","","Immediately rectified when pointed out by the inspector. Training carried out to all deck officer and crew.","2020-11-30","","Completed","2020-11-30","No","No","No","External"]
[null,null,null,null,16879,"46_19/12/2020 5:31:09 AM","2020-12-01","Defect","Ship Staff","Ship Staff Insp.","AE # 3 PRIMING PUMP LEAKING FROM MECHINICAL SEAL.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","AE # 3 PRIMING PUMP TO OVERHAUL AND MECHINICAL SEAL TO RENEW.","2020-12-30","","Completed","2020-12-16","No","No","No","Internal"]
[null,null,null,null,16882,"46_04/01/2021 5:23:47 AM","2020-12-01","Defect","Ship Staff","Ship Staff Insp.","EJECTOR PUMP SUCTION VALVE LEAKING FROM THE GALND.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","EJECTOR PUMP SUCTION VALVE GLAND PACKING TO BE RENEWED.","2020-12-30","","Completed","2020-12-08","No","No","No","Internal"]
[null,null,null,null,15666,"46_16/12/2020 9:59:18 AM","2020-12-02","Critical Equipment","Ship Staff","Ship Staff Insp.","Target Echoes Suddenly disappeared in S-Band Radar Monitor","Navigation - RADAR","Navigation","Equipment Related","4.2","Medium","","","Swiitch Off Radar and Checked Scanner Unit for any water ingress, loose connection, PCB, gear encoder and motor for any abnormal noice and burnt. Same Reported to Office and requested for Shore's Service Assistance.","2020-12-30","WRUB205116 - S-Band Radar Repair","Completed","2020-12-09","No","No","No","Internal"]
[null,null,null,null,16884,"46_19/12/2020 5:39:28 AM","2020-12-03","Defect","Ship Staff","Ship Staff Insp.","HFO # 1 PURIFIER OPERATING WATER REDUCER LEAKING FROM DIAPHGRAM.","E/R - Purifier","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","HFO # 1 PURIFER OPERATING WATER REDUCING ASSEMBLY TO OVERHAUL.","2020-12-30","","Completed","2020-12-17","No","No","No","Internal"]
[null,null,null,null,16885,"46_04/01/2021 5:34:12 AM","2020-12-03","Defect","Ship Staff","Ship Staff Insp.","THE ATMOSPHERIC CONDENSOR FILTER CASING HAVING HOLE / SOFT PATCH.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","THE NEW FILTER CASING NEEDS TO BE REPLACED FOR ATMOSPHERIC CONDENSOR.","2021-01-31","","Completed","2020-12-29","No","No","No","Internal"]
[null,null,null,null,16886,"46_04/01/2021 5:44:55 AM","2020-12-04","Defect","Ship Staff","Ship Staff Insp.","EJECTOR PUMP DISCHARGE VALVE LEAKING FROM GLAND.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","EJECTOR PUMP DISCHARGE VALVE GLAND PACKING NEEDS TO BE REPLACED.","2021-01-15","","Completed","2021-01-03","No","No","No","Internal"]
[null,null,null,null,16887,"46_04/01/2021 5:28:01 AM","2020-12-06","Defect","Ship Staff","Ship Staff Insp.","AE # 1 SEAL POT PIPE BROKEN.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","AE # 1 NEW SEAL POT PIPE NEEDS TO BE FABRICATED.","2020-12-30","","Completed","2020-12-22","No","No","No","Internal"]
[null,null,null,null,16888,"46_04/01/2021 5:36:36 AM","2020-12-08","Critical Equipment","Ship Staff","Ship Staff Insp.","PORT SIDE LIFE BOAT BATTERY EXPIRED.","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","THE REQUESTION HAS BEEN RAISED. ONCE RECIEVE REPLACE THE BATTERY.","2020-12-30","","Completed","2020-12-28","No","No","No","Internal"]
[null,null,null,null,15626,"46_28/11/2020 6:32:36 PM","2020-12-15","Defect","Ship Staff","Ship Staff Insp.","AE# 1 FLYWHEEL GEAR TEETH (RING GEAR) FOR STARTING AIR MOTOR WORN OUT.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","THE AE # 1 FLYWHEEL GEAR TEETH (RING GEAR) RENEWED WITH NEW SPARE ","2021-01-15","","Completed","2021-01-12","No","No","No","Internal","shore serivce arrange at india to assist in changing the flywheel"]
[null,null,null,null,16889,"46_19/12/2020 5:25:42 AM","2020-12-17","Defect","Ship Staff","Ship Staff Insp.","PORT SIDE AE JACKET WATER COOLER INLET PIPE HAVING SOFT PATCH.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.31","Very High","","","PORT SIDE JACKET WATER COOLER NEW INLET PIPE NEEDS TO BE FABRICATED.","2021-01-30","","Completed","2021-01-02","No","No","No","Internal"]
[null,null,null,null,16890,"46_04/01/2021 5:42:31 AM","2020-12-17","Defect","Ship Staff","Ship Staff Insp.","STBD SIDE AE JACKET WATER COOLER SEA WATER INLET LINE HAVING PIN HOLE AND SOFT PATCH.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","THE STBD AE JACKET WATER COOLER SEA WATER INLET LINE NEEDS TO BE FABRICATED / LEAK TO BE RECTIFIED BY WELDING.","2021-01-15","","Completed","2021-01-03","No","No","No","Internal"]
[null,null,null,null,15034,"46_15/11/2020 7:16:42 PM","2020-12-18","Defect","Ship Staff","Ship Staff Insp.","ECR AC SEA WATER INLET LINE AFTER VALVE HAVING PIN HOLE.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","ECR AC SEA WATER LEAKAGE RECTIFIED ","2021-01-30","","Completed","2021-01-14","No","No","No","Internal","to carry out first available oppurtunity"]
[null,null,null,null,16891,"46_04/01/2021 5:31:21 AM","2020-12-19","Defect","Ship Staff","Ship Staff Insp.","WASTE OIL INCINERATOR SLUDGE  PUMP AND MOTOR IS NOT OPERATIONAL.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","THE REQUESTION FOR WASTE OIL INCINERATOR SLUDGE PUMP AND MOTOR HAS BEEN RAISED. ONCE SUPPLIED REPLACE THE SAME.","2020-12-30","","Completed","2020-12-28","No","No","No","Internal"]
[null,null,null,null,15625,"46_28/11/2020 6:38:50 PM","2020-12-22","Defect","Ship Staff","Ship Staff Insp.","THE AUXILARY BOILER FUEL OIL FLOWMETER NOT OPERATIONAL.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","THE NEW AUXILARY BOILER FUEL OIL FLOWMETER REPLACED AND TRIED OUT FOUND IN GOOD ORDER.","2021-01-31","","Completed","2021-01-28","No","No","No","Internal","spares delivered to vessel, awaiting suitable opportunity"]
[null,null,null,null,15037,"46_15/11/2020 7:06:46 PM","2020-12-22","Defect","Ship Staff","Ship Staff Insp.","THE AUXILARY ENGINE OUTLET FUEL OIL FLOWMETER NOT OPERATIONAL.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","SHIP STAFF TRIED TO OVERHAULED AT PRESENT IT WAS FOUND IN ORDER. WILL CLOSELY MONITOR ","2021-02-28","","Completed","2021-01-31","No","No","No","Internal","order new parts if not able to rectify after ohauling"]
[null,null,null,null,16908,"46_Sat Jan 09 2021 09:13:56 GMT+0000","2020-12-25","Observation","Owner / Marine / Tech. Suptd.","Nav Audit / Verification","Mooring arrangement Plan was not discussed with pilot and same not highlighted in the master pilot exchange for last discharge port in line with MSMP","Navigation - Others","Navigation","Knowledge Based","","","","","Briefing of bridge team to be carried out to avoid a repeat of this in the future.","2021-03-21","","Completed","2020-12-27","No","No","No","Internal"]
[null,null,null,null,16892,"46_04/01/2021 5:39:23 AM","2020-12-29","Defect","Ship Staff","Ship Staff Insp.","AUXILARY ENGINE SEA WATER COOLING PUMP MOTOR IS GIVING ABNORMAL NOISE AND VIBRATION.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","THE AUXILARY ENGINE SEA WATER COOLING PUMP MOTOR TO BE OVERHAULED.","2021-01-15","","Completed","2021-01-01","No","No","No","Internal"]
[null,null,null,null,18178,"46_16/1/2021 10:14:39 AM","2021-01-11","Defect","Ship Staff","Ship Staff Insp.","Stbd side Emcy shower found leaking","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.61","Low","","","The leak rectified and the unit tested.","2021-01-12","","Completed","2021-01-12","No","No","No","Internal"]
[null,null,null,null,18179,"46_28/1/2021 11:08:50 AM","2021-01-14","Non Conformity","Ship Staff","Ship Staff Insp.","CRACK DISCHARGE HOSES OF PORTABLE DCP FIRE EXTINGUISHERS.","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.42","Medium","","","ALL CRACK DISCHARGE HOSES CHANGED WITH NEW SPARE HOSES. \n\nINSPECTION PROCEDURES AS PER MANUFACTURE'S GUIDELINE POSTED IN VICINITY OF EACH EXTINGUISHER.","2021-03-15","","Completed","2021-01-16","No","No","No","Internal"]
[null,null,null,null,15031,"46_08-Nov-20 10:01:26 AM","2021-01-17","Observation","Ship Staff","Ship Staff Insp.","Accommodation cleaning to carry out & plan for painting white colour to get more luminance, CCR bulkheads to be cleaned","Accommodation","General Appearance","Equipment Related","","","","","ACCOMMODATION & CCR BULKHEAD CLEANED/ CCR FLOOR PAINTED. REQUISITION RAISED FOR SIGMARINE WHITE PAINT.","2021-03-28","","Completed","2021-03-07","Yes","No","No","Internal","order new light shades if required"]
[null,null,null,null,18180,"46_31-Jan-21 2:08:26 PM","2021-01-18","Defect","Ship Staff","Ship Staff Insp.","Tank cleaning heater thermometers found defective and showing wrong readings.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.18","Low","","","Replaced with new thermometers.","2021-03-25","","Completed","2021-01-21","No","No","No","Internal"]
[null,null,null,null,18181,"46_31-Jan-21 4:10:08 PM","2021-01-20","Defect","Ship Staff","Ship Staff Insp.","Steam leaking from non return valve flange of inlet line in pump room. ","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","11.4","Very High","","","Steam gasket to be replaced and flange to be tightened.","2021-03-25","","Completed","2021-02-22","No","No","No","Internal"]
[null,null,null,null,18182,"46_30/01/2021 7:11:16 PM","2021-01-30","Defect","Ship Staff","Ship Staff Insp.","aux engine  ht wter cooler sea water line has pin hole","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","pipe section to be taken to workshop and repair carried out","2021-02-10","","Completed","2021-02-12","No","No","No","Internal"]
[null,null,null,null,18183,"46_30/01/2021 7:08:36 PM","2021-01-30","Defect","Ship Staff","Ship Staff Insp.","Atmospheric condensor sea wtr inlet line has pin hole","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","pipe  taken to workshop and repaired","2021-02-10","","Completed","2021-02-05","No","No","No","Internal"]
[null,null,null,null,18184,"46_30/01/2021 7:13:52 PM","2021-01-30","Defect","Ship Staff","Ship Staff Insp.","accomodation ac sea water inlet pipe in engine room has pin hole","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","pipe section  taken to workshop and repaired","2021-02-10","","Completed","2021-02-05","No","No","No","Internal"]
[null,null,null,null,18185,"46_31/01/2021 9:13:32 AM","2021-01-31","Defect","Ship Staff","Ship Staff Insp.","ACCOMODATION AIR CONDITION PLANT COMPRESSOR NO.2 HIGH PRESSURE DISCHARGE LINE HAS LEAK","E/R - Aux. Mach.,E/R - Pipes/ valves & fittings,Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","ISOLATED THE NO.2 COMPRESSOR AND DEPRESSURIZED THE LINES,  RECTFIED THE LEAK","2021-02-10","","Completed","2021-02-09","No","No","No","Internal"]
[null,null,null,null,18186,"46_15-Feb-21 9:26:56 AM","2021-02-01","Defect","Ship Staff","Ship Staff Insp.","5S COT Tank dome hook eye plate thinned down.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.18","Low","","","To dismantle the part and weld a new eye plate in workshop.","2021-04-15","","Completed","2021-02-07","No","No","No","Internal"]
[null,null,null,null,18187,"46_14/02/2021 6:49:14 AM","2021-02-01","Defect","Ship Staff","Ship Staff Insp.","AE #3 running hour meter not working","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Defective running hour counter replaced with new hour meter received at singapore on 08Feb 2021.","2021-02-20","","Completed","2021-02-13","No","No","No","Internal"]
[null,null,null,null,18188,"46_15/02/2021 8:06:11 AM","2021-02-15","Defect","Ship Staff","Ship Staff Insp.","Economiser soot blowing steam valve gland leakage","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","gland of valve changed. Leak rectified.","2021-02-25","","Completed","2021-02-26","No","No","No","Internal"]
[null,null,null,null,18784,"46_15/03/2021 7:54:15 PM","2021-02-15","Non Conformity","Ship Staff","Ship Staff Insp.","One of the lifejacket found with method of securing to the wearer required tying of knots. Not complying with requirements of LSA Code 2.2.1.5.4","LSA / FFA","Safety / LSA / FFA","Knowledge Based","5.32","High","","","Immediately removed the non-compliant Lifejacket and marked with \"not in use\" and replaced with new spare lifejacket in compliance with the code and discuss on upcoming safety meeting","2021-04-15","","Completed","2021-02-20","No","No","No","Internal"]
[null,null,null,null,18174,"46_15/02/2021 7:59:21 AM","2021-02-15","Defect","Ship Staff","Ship Staff Insp.","Aux Eng#1 Exhaust trunking bellow Found exhaust gas leakage","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","exhaust bellow replaced with spare one.","2021-03-15","","Completed","2021-03-16","No","No","No","Internal"]
[null,null,null,null,18175,"46_15/02/2021 8:02:55 AM","2021-02-15","Defect","Ship Staff","Ship Staff Insp.","Aux Eng# 2 cooling water line ,needle purging valve and expansion tank line valve found leakage.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","valves replaced with spare valves received.","2021-03-15","WRUB210051","Completed","2021-03-26","No","No","No","Internal","Plan to renew once received the v/v"]
[null,null,null,null,18176,"46_28/02/2021 3:53:39 PM","2021-02-28","Defect","Ship Staff","Ship Staff Insp.","AE#3 Oil max centrifuge filter inlet hose oil leakage.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","lube oil Hose renewed with spare new hose received.","2021-03-30","","Completed","2021-03-25","No","No","No","Internal"]
[null,null,null,null,18785,"46_15-Mar-21 5:38:00 PM","2021-03-01","Defect","Ship Staff","Ship Staff Insp.","Hawse pipe railing damaged and broken due to heavy weather.","Deck - Mooring Machinery","Mooring","External Factors","9.2","Very High","","","Plan to weld the broken and damged railing during gas free condition.","2021-05-02","","Completed","2021-03-11","No","No","No","Internal"]
[null,null,null,null,18786,"46_15/03/2021 9:08:52 AM","2021-03-15","Defect","Ship Staff","Ship Staff Insp.","ECR AC SEA WATER INLET LINE PIPE LEAKAGE","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","PIPELINE  RENEWED.","2021-03-30","","Completed","2021-03-15","No","No","No","Internal"]
[null,null,null,null,null,"46_15/03/2021 7:19:29 AM","2021-03-15","Defect","Ship Staff","Ship Staff Insp.","ECR PLATFORM FIRE HYDRANT VALVE  LEAKAGE","LSA / FFA","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","New Valve fitted and the defect rectified","2021-05-25","WRUB210028","Completed","2021-05-14","No",null,null,"Internal"]
[null,null,null,null,null,"46_28/11/2020 6:34:08 PM","2021-03-18","Defect","Ship Staff","Ship Staff Insp.","THE MAIN ENGINE SHAFT POWER METER NOT OPERATIONAL. ITS NOT CALCULATING POWER ONLY SHOWS THE RPM.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Noticed working. Showing RPM as well as Power","2021-06-18",null,"Completed","2021-05-14","No",null,null,"Internal"]
[null,null,null,null,18787,"46_26/03/2021 10:24:31 PM","2021-03-24","Observation","Owner / Marine / Tech. Suptd.","ISM Audit","Hospital has a damaged chair same to be removed","Miscellaneous","MLC Related","Knowledge Based","11.15","Low","","","Removed the damaged chair from the hospital and put in scrapped storage for next disposal ashore. Briefed all officer and crew the hazards and consequences that put into danger the person will use and may create injury to the person. Advised to all crew onward all damaged chair to discards and put to proper place where cannot be use and for disposal ashore.","2021-06-23","","Completed","2021-03-28","No","No","No","Internal"]
[null,null,null,null,18788,"46_26/03/2021 10:31:10 PM","2021-03-24","Observation","Owner / Marine / Tech. Suptd.","Nav Audit / Verification","Magnetic Compass found with bubble","Navigation - Others","Navigation","Human Error","4.9","Medium","","","Removed bubbles in the Magnetic Compass. Briefed officer in-charge to thoroughly check and make sure Magnetic Compass is free from bubbles at all times and strict compliance of vessel PMS onward.","2021-06-23","","Completed","2021-03-28","No","No","No","Internal"]
[null,null,null,null,18789,"46_26/03/2021 10:06:21 PM","2021-03-24","Observation","Owner / Marine / Tech. Suptd.","ISM Audit","Hawse pipe cover was not in place. Vessel was riding on stbd anchor","Miscellaneous","ISPS Related","Knowledge Based","7.12","High","","","Hawse pipe cover in place when pointed out. Briefed all officer and crew the importance to cover the hawse pipe after anchoring to avoid security breach via hawse pipe and for stirct compliance onward.","2021-06-23","","Completed","2021-03-28","No","No","No","Internal"]
[null,null,null,null,18790,"46_25/03/2021 6:10:36 PM","2021-03-24","Observation","Owner / Marine / Tech. Suptd.","ISM Audit","SMPEP wilden was not in state of readiness during the bunkering operations","Miscellaneous","Emgcy. Systems","Human Error","6.3","Low","","","SMPEP wilden pump put in place at the time pointed out. Training/brief to all personnel to avoid recurrence.","2021-06-23","","Completed","2021-03-28","No","No","No","Internal"]
[null,null,null,null,18791,"46_25/03/2021 6:20:05 PM","2021-03-24","Observation","Owner / Marine / Tech. Suptd.","ISM Audit","Drums stored in the midship were not lashed properly","Miscellaneous","General Appearance","Knowledge Based","5.11","Low","","","Square-up and secured/lashed properly. Brief/discuss to all personnel to make sure all moving items on deck and engine to secure properly at all times without failure accordingly.","2021-06-23","","Completed","2021-03-28","No","No","No","Internal"]
[null,null,null,null,18792,"46_26/03/2021 9:59:51 PM","2021-03-24","Observation","Owner / Marine / Tech. Suptd.","ISM Audit","STS Plan records to update in STS file","Documentation","Cert. & Docu.","Knowledge Based","8.54","Medium","","","Corporate the STS Plan and STS file in one file/folder to avoid misplace check lists files of previous STS operations dated 18 Feb 2018. Since then no STS operations carry out.","2021-06-23","","Completed","2021-03-28","No","No","No","Internal"]
[null,null,null,null,18793,"46_26/03/2021 9:43:04 PM","2021-03-24","Observation","Owner / Marine / Tech. Suptd.","ISM Audit","Shore Familiarization form was not completed for technician attnded in Singapore","Documentation","Cert. & Docu.","Behaviour Based","5.12","Medium","","","Brief all officer and crew to make sure to complete the shore familiarization form prior the shore contractor to proceed on their purpose onboard and after completing the form to make sure to put in place in respective file right away to avoid misplace the form onward.","2021-06-23","","Completed","2021-03-28","No","No","No","Internal"]
[null,null,null,null,18794,"46_01/04/2021 12:39:21 AM","2021-03-30","Observation","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","No. 5 Stb'd Forward entrance manhole cover was removed for sighting the tank from deck level, and observed few intermittent scales built up on the sides of the vertical descending ladder.","Hull & Tanks","Cargo / Ballast Systems","Equipment Related","2.16","Medium","","","Derusted and repainted the few intermittent scales built up on the sides of  the vertical descending ladder ","2021-06-29","","Completed","2021-03-31","No","No","No","External"]
[null,null,null,null,18795,"46_01/04/2021 12:49:52 AM","2021-03-30","Observation","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","The latest foam sample analysis certificates for the alcohol resistant foam on board did not indicate a stability test with acetone.","LSA / FFA","Safety / LSA / FFA","External Factors","5.36","Low","","","Advised to the office to request revised certificate with require stability test with acetone mention on the certificate.","2021-06-29","","Completed","2021-03-31","No","No","No","External"]
[null,null,null,null,18796,"46_01/04/2021 1:01:03 AM","2021-03-30","Observation","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","The cargo deck area aft spill pumps when tested did not function. The deck compressor located in the fore peak store had tripped. The compressor was reset and restarted, after which the spill pumps were tested and in good order.","Miscellaneous","MARPOL Related","Equipment Related,Knowledge Based","6.3","Low","","","Further investigate the cause of Deck Air Compressor tripped","2021-06-29","","Completed","2021-03-31","No","No","No","External"]
[null,null,null,null,18797,"46_01/04/2021 1:08:40 AM","2021-03-30","Observation","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","The decontamination shower and eye wash arrangement in way of and top of the platform at manifold area was not suitably marked or pathway highlighted from either side of the cargo manifold.","Miscellaneous","Safety / LSA / FFA","Knowledge Based","8.61","Low","","","Advised to office as the decontamination shower and eye wash is distinctly marked with shower symbols.","2021-06-29","","Completed","2021-03-30","No","No","No","External"]
[null,null,null,null,18802,"46_01/04/2021 12:55:34 AM","2021-03-30","Observation","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","It was observed that apron was not part of the PPE available in the paint locker. This observation was rectified prior to end of closing meeting","Miscellaneous","Safety / LSA / FFA","Human Error","5.46","Medium","","","In place the required apron in the paint locker when observation pointed out.","2021-06-29","","Completed","2021-03-30","No","No","No","External"]
[null,null,null,null,null,"46_15/04/2021 6:17:34 AM","2021-04-01","Breakdown","Ship Staff","Ship Staff Insp.","Main Cooling Sea Water Pump is non-operational due to burnt Motor.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Motor fitted in Place. Confirmation on terminal connection rec'd from the office on 7th June'21 and work was completed and tried out on 8th June'21.","2021-06-15","WRUB210086","Completed","2021-06-08","No",null,null,"Internal"]
[null,null,null,null,18798,"46_28-Apr-21 9:08:44 PM","2021-04-05","Observation","Ship Staff","Ship Staff Insp.","1P STBD MANIFOLD VALVE FOUND LEAKING DURING TANK CLEANING OPERATION.","Cargo Mach.,Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.41","Very High","","","1P STBD MANIFOLD VALVE REMOVED SS & TEFLON SEAT RING RENEWED. MANIFOLD VALVE FITTED IN PLACE & PRESSURE TESTED. IN ORDER","2021-05-06","","Completed","2021-04-06","No","No","No","Internal"]
[null,null,null,null,18799,"46_28-Apr-21 9:12:22 PM","2021-04-07","Observation","Ship Staff","Ship Staff Insp.","PORT SIDE CARGO MANIFOLD 3 PRESSURE GAUGE FOUND FAULTY","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related,External Factors","8.41","Very High","","","ALL 3 MANIFOLD PRESSURE GAUGE RENEWED.","2021-05-10","","Completed","2021-04-10","No","No","No","Internal"]
[null,null,null,null,18800,"46_28-Apr-21 9:23:50 PM","2021-04-08","Observation","Ship Staff","Ship Staff Insp.","STBD PLASTIC GARBAGE CONTAINER COVER FOUND BROKEN.","Accommodation,Miscellaneous","General Appearance","External Factors","6.2","High","","","NEW COVER FABRICATED & FIXED IN PLACE.","2021-05-08","","Completed","2021-04-24","No","No","No","Internal"]
[null,null,null,null,18801,"46_28-Apr-21 9:17:45 PM","2021-04-10","Non Conformity,Observation","Ship Staff","Ship Staff Insp.","TOTAL 9 WEATHER TIGHT DOORS RUBBER PACKING FOUND CRAKED & DAMAGE AT MULTIPLE LOCATION.","Accommodation","Structural Condn. / WT integrity ","External Factors","11.6","Medium","","","ALL WEATHER TIGHT DOORS CHALK TEST CARRIED OUT & 9 DOORS RUBBER PACKING RENEWED.","2021-05-10","","Completed","2021-04-24","No","No","No","Internal"]
[null,null,null,null,null,"46_15/03/2021 8:04:55 AM","2021-04-15","Defect","Ship Staff","Ship Staff Insp.","Air Handling Unit Thermostat malfunctioning which prevents the compressor from cut in","Accommodation,Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","New spare Thermostat fitted and found working.","2021-05-15","WRUB210047","Completed","2021-06-05","No",null,null,"Internal"]
[null,null,null,null,null,"46_28/04/2021 4:45:29 PM","2021-04-24","Defect","Ship Staff","Ship Staff Insp.","N2 ROOM LOW O2 ALARM BUZZER FOUND DEFECTIVE","Elect. Mach. & Equip.,Miscellaneous","Cargo / Ballast Systems","Equipment Related",8.3800000000000008,"Low","Not Applicable","Not Applicable","New spare sensor and siren fitted. working normal.","2021-05-12","WRUB210004","Completed","2021-06-05","No",null,null,"Internal"]
[null,null,null,null,null,"46_28-Apr-21 9:30:11 PM","2021-04-25","Observation","Ship Staff","Ship Staff Insp.","MAIN DECK CATWALK GRATING NEAR MIDSHIP CRANE AREA FOUND DAMAGE / BROKEN.","Deck - Pipe / Fittings","General Appearance","Equipment Related,External Factors",11.1,"High","Not Applicable","Not Applicable","NEW SPARE GRATING CUT FOR THE SIZE AND FITTED IN PLACE.","2021-05-12",null,"Completed","2021-04-30","No",null,null,"Internal"]

{"sheet":"Calc","index":2,"n_rows":28,"n_cols":12,"rows_kept":28,"cut":false,"hidden":true,"merged":[]}
["Def_type","Def_cause","Equipments","VIQrefno","Observer_code"]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,"Dim itemSele As Long"]
[null,null,null,null,null,null,null,null,null,null,null,"   dim startRow as integer"]
[null,null,null,null,null,null,null,null,null,null,null,"   startRow=1"]
[null,null,null,null,null,null,null,null,null,null,null,"        For itemSele = 0 To ListBox1.ListCount - 1"]
[null,null,null,null,null,null,null,null,null,null,null,"        If ListBox1.Selected(itemSele) = True Then"]
[null,null,null,null,null,null,null,null,null,null,null,"        Worksheets(\"WorksheetName\").Range(\"A\" & startRow).Value = ListBox1.List(itemSele)"]
[null,null,null,null,null,null,null,null,null,null,null,"        startRow = startRow + 1"]
[null,null,null,null,null,null,null,null,null,null,null,"        End If"]
[null,null,null,null,null,null,null,null,null,null,null,"        Next"]
[null,null,null,null,null,null,null,null,null,null,null,"Dim LastRowA As String"]
[null,null,null,null,null,null,null,null,null,null,null,"        Dim itemSele As Long"]
[null,null,null,null,null,null,null,null,null,null,null,"       Dim startRow as integer"]
[null,null,null,null,null,null,null,null,null,null,null,"        LastRowA = ActiveSheet.Cells(Rows.count, \"A\").End(xlUp).row"]
[null,null,null,null,null,null,null,null,null,null,null,"        startQue = 0"]
[null,null,null,null,null,null,null,null,null,null,null,"        For itemSele = 0 To ListBox1.ListCount - 1"]
[null,null,null,null,null,null,null,null,null,null,null,"        For startRow = 1 To LastRowA"]
[null,null,null,null,null,null,null,null,null,null,null,"        If Worksheets(\"WorksheetName\").Range(\"A\" & startRow).Value = ListBox1.List(itemSele) Then"]
[null,null,null,null,null,null,null,null,null,null,null,"        ListBox1.Selected(itemSele) = True"]
[null,null,null,null,null,null,null,null,null,null,null,"        Exit For"]
[null,null,null,null,null,null,null,null,null,null,null,"        End If"]
[null,null,null,null,null,null,null,null,null,null,null,"        Next j"]
[null,null,null,null,null,null,null,null,null,null,null,"        Next"]
[null,null,null,null,null,null,null,null,null,null,null,"        End If"]

{"sheet":"Areaofobs","index":3,"n_rows":17,"n_cols":2,"rows_kept":17,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Cargo / Ballast Systems",11]
["Cert. & Docu.",2]
["Communication",6]
["Crew Management",3]
["Emgcy. Systems",13]
["Eng. / Strg. Comp.",14]
["General Appearance",15]
["Ice Opns.",17]
["ISM Related",7]
["ISPS Related",10]
["MARPOL Related",9]
["MLC Related",4]
["Mooring",12]
["Navigation",5]
["Safety / LSA / FFA",8]
["Structural Condn. / WT integrity ",16]

{"sheet":"Vessel_type","index":4,"n_rows":1,"n_cols":2,"rows_kept":1,"cut":false,"hidden":true,"merged":[]}
["Vessel_type","ID"]

{"sheet":"Deficiency_type","index":5,"n_rows":8,"n_cols":3,"rows_kept":8,"cut":false,"hidden":true,"merged":[]}
["TITLE","Type of deficiency_description","ID"]
["Breakdown",null,6]
["Critical Equipment",null,4]
["Defect",null,1]
["Guarantee Claim",null,8]
["Non Conformity",null,2]
["Observation",null,3]
["Other",null,7]

{"sheet":"VIQrefno","index":6,"n_rows":363,"n_cols":3,"rows_kept":363,"cut":false,"hidden":true,"merged":[]}
["VIQ_ref_no","Risk Value of observation","ID"]
["1.1","Low",8627]
["1.10","Low",8636]
["1.11","Low",8637]
["1.12","Low",8638]
["1.13","Low",8639]
["1.14","Low",8640]
["1.15","Low",8641]
["1.16","Low",8643]
["1.17","Low",8644]
["1.18","Low",8645]
["1.19","Low",8646]
["1.2","Low",8628]
["1.20","Low",8647]
["1.21","",8648]
["1.22","Low",8650]
["1.23","Low",8651]
["1.24","Low",8652]
["1.25","Low",8653]
["1.26","Low",8654]
["1.3","Low",8629]
["1.4","Low",8630]
["1.5","Low",8631]
["1.6","Low",8632]
["1.7","Low",8633]
["1.8","Low",8634]
["1.9","Low",8635]
["1.99","High",15785]
["10.1","Medium",8821]
["10.10","High",8830]
["10.11","Medium",8831]
["10.12","Very High",8832]
["10.13","Very High",8833]
["10.14","Medium",8834]
["10.15","Low",8835]
["10.16","Very High",8836]
["10.17","Very High",8837]
["10.18","High",8838]
["10.19","Very High",8839]
["10.2","Low",8822]
["10.20","High",8840]
["10.21","Medium",8841]
["10.22","Low",8842]
["10.23","Medium",8843]
["10.24","Low",8844]
["10.25","Very High",8845]
["10.26","High",8846]
["10.27","Medium",8847]
["10.28","Low",8848]
["10.29","Medium",8849]
["10.3","Medium",8823]
["10.30","High",8850]
["10.31","Very High",8851]
["10.32","Very High",8852]
["10.33","High",8853]
["10.34","High",8854]
["10.35","Very High",8855]
["10.36","Very High",8856]
["10.37","Medium",8857]
["10.38","Medium",8858]
["10.39","High",8859]
["10.4","High",8824]
["10.40","Medium",8860]
["10.41","Medium",8861]
["10.42","Medium",8862]
["10.43","Medium",8863]
["10.44","Medium",8864]
["10.45","Very High",8865]
["10.46","High",8866]
["10.47","Medium",8867]
["10.48","High",8868]
["10.49","Medium",8869]
["10.5","Low",8825]
["10.50","High",8870]
["10.51","Low",8871]
["10.52","Medium",8872]
["10.53","Medium",8873]
["10.54","High",8874]
["10.55","Low",8875]
["10.6","Very High",8826]
["10.7","Medium",8827]
["10.8","Medium",8828]
["10.9","Medium",8829]
["10.99","High",8876]
["11.1","High",8780]
["11.10","Medium",8789]
["11.11","Very High",8790]
["11.12","Low",8791]
["11.13","Low",8792]
["11.14","Medium",8793]
["11.15","Low",8794]
["11.16","Low",8795]
["11.17","Low",8796]
["11.2","Medium",8781]
["11.3","Medium",8782]
["11.4","Very High",8783]
["11.5","Medium",8784]
["11.6","Medium",8785]
["11.7","High",8786]
["11.8","Low",8787]
["11.9","Low",8788]
["11.99","High",8797]
["12.1","High",8798]
["12.10","High",8808]
["12.11","High",8809]
["12.12","High",8810]
["12.13","High",8811]
["12.14","High",8812]
["12.15","High",8813]
["12.16","High",8814]
["12.17","High",8815]
["12.18","High",8816]
["12.19","High",8817]
["12.2","High",8799]
["12.20","High",8818]
["12.21","High",8819]
["12.3","High",8801]
["12.4","High",8802]
["12.5","High",8803]
["12.6","High",8804]
["12.7","High",8805]
["12.8","High",8806]
["12.9","High",8807]
["12.99","High",8820]
["2.1","Very High",15]
["2.1.9","Very High",16]
["2.10","Medium",25]
["2.11","Medium",26]
["2.12","Medium",27]
["2.13","High",28]
["2.14","High",29]
["2.15","High",30]
["2.16","Medium",31]
["2.2","Medium",17]
["2.3","High",18]
["2.4","Medium",19]
["2.5","Low",20]
["2.6","Medium",21]
["2.7","High",22]
["2.8","Medium",23]
["2.9","Low",24]
["2.99","High",8672]
["3.1","High",8673]
["3.2","Very High",8674]
["3.3","High",8675]
["3.4","Low",8655]
["3.5","Medium",8676]
["3.6","High",8677]
["3.7","Very High",8678]
["3.8","Very High",8679]
["3.99","High",8680]
["4.1","High",8681]
["4.10","High",8690]
["4.11","Medium",8691]
["4.12","Very High",8692]
["4.13","Very High",8693]
["4.14","Very High",8694]
["4.15","Very High",8695]
["4.16","Very High",8696]
["4.17","Very High",8697]
["4.18","Very High",8698]
["4.19","Low",8699]
["4.2","Medium",8682]
["4.20","Very High",8700]
["4.21","High",8701]
["4.22","Low",8702]
["4.23","High",8703]
["4.24","High",8704]
["4.25","Low",8705]
["4.26","Low",8706]
["4.27","High",8707]
["4.3","Medium",8683]
["4.4","High",8684]
["4.5","Very High",8685]
["4.6","Medium",8686]
["4.7","High",8687]
["4.8","Medium",8688]
["4.9","Medium",8689]
["4.99","High",8708]
["5.1","Very High",8877]
["5.10","High",8886]
["5.11","Low",8887]
["5.12","Medium",8888]
["5.13","High",8889]
["5.14","Very High",8890]
["5.15","Medium",8891]
["5.16","Medium",8892]
["5.17","Very High",8893]
["5.18","High",8894]
["5.19","Medium",8895]
["5.2","Very High",8878]
["5.20","Medium",8896]
["5.21","Medium",8897]
["5.22","High",8899]
["5.23","Very High",8900]
["5.24","Very High",8901]
["5.25","Medium",8902]
["5.26","Medium",8903]
["5.27","Medium",8904]
["5.28","Very High",8905]
["5.29","High",8906]
["5.3","Low",8879]
["5.30","High",8907]
["5.31","High",8908]
["5.32","High",8909]
["5.33","High",8910]
["5.34","Low",8911]
["5.35","Medium",8912]
["5.36","Low",8913]
["5.37","Low",8914]
["5.38","High",8915]
["5.39","Very High",8916]
["5.4","High",8880]
["5.40","Very High",8917]
["5.41","Very High",8918]
["5.42","Medium",8919]
["5.43","High",8920]
["5.44","High",8921]
["5.45","Medium",8924]
["5.46","Medium",8925]
["5.47","Low",8926]
["5.48","Medium",8927]
["5.5","Low",8881]
["5.6","Low",8882]
["5.7","Medium",8883]
["5.8","Medium",8884]
["5.9","Very High",8885]
["5.99","High",8928]
["6.1","Medium",8709]
["6.10","Low",8718]
["6.11","High",8719]
["6.12","Medium",8720]
["6.13","Low",8721]
["6.14","High",8722]
["6.15","High",8723]
["6.16","Very High",8724]
["6.17","Very High",8725]
["6.18","Medium",8726]
["6.19","Low",8727]
["6.2","High",8710]
["6.20","Medium",8728]
["6.21","High",8729]
["6.22","Medium",8730]
["6.3","Low",8711]
["6.4","High",8712]
["6.5","Low",8713]
["6.6","Medium",8714]
["6.7","High",8715]
["6.8","High",8716]
["6.9","Low",8717]
["6.99","High",8731]
["7.1","High",8732]
["7.10","High",8741]
["7.11","High",8742]
["7.12","High",8743]
["7.13","Medium",8744]
["7.14","Medium",8745]
["7.15","High",8746]
["7.16","High",8747]
["7.17","High",8748]
["7.2","High",8733]
["7.3","Low",8734]
["7.4","Low",8735]
["7.5","Low",8736]
["7.6","Medium",8737]
["7.7","Low",8738]
["7.8","High",8739]
["7.9","High",8740]
["7.99","High",8749]
["8.1","Very High",8929]
["8.10","Very High",8938]
["8.11","Medium",8939]
["8.12","Medium",8940]
["8.13","Low",8941]
["8.14","Medium",8942]
["8.15","Medium",8943]
["8.16","Medium",8944]
["8.17","Medium",8945]
["8.18","Low",8946]
["8.19","Medium",8947]
["8.2","Medium",8930]
["8.20","Medium",8948]
["8.21","Medium",8949]
["8.22","Very High",8950]
["8.23","Medium",8951]
["8.24","Very High",8952]
["8.25","Medium",8953]
["8.26","Low",8954]
["8.27","Medium",8955]
["8.28","Medium",8956]
["8.29","Medium",8958]
["8.3","Medium",8931]
["8.30","Very High",8959]
["8.31","Medium",8960]
["8.32","Medium",8961]
["8.33","Very High",8962]
["8.34","High",8963]
["8.35","Medium",8964]
["8.36","Medium",8965]
["8.37","Medium",8967]
["8.38","Low",8968]
["8.39","Low",8969]
["8.4","Very High",8932]
["8.40","Very High",8970]
["8.41","Very High",8971]
["8.42","Medium",8972]
["8.43","Low",8973]
["8.44","Medium",8975]
["8.45","High",8976]
["8.46","Medium",8977]
["8.47","Medium",8978]
["8.48","Medium",8979]
["8.49","Medium",8980]
["8.5","Medium",8933]
["8.50","Very High",8981]
["8.51","Very High",8982]
["8.52","Very High",8983]
["8.53","Very High",8984]
["8.54","Medium",8985]
["8.55","Very High",15711]
["8.56","Very High",15712]
["8.57","Medium",15713]
["8.58","Medium",15714]
["8.59","Very High",15715]
["8.6","Medium",8934]
["8.60","Medium",15716]
["8.61","Low",15717]
["8.62","Medium",15718]
["8.63","Medium",15719]
["8.7","Very High",8935]
["8.8","Very High",8936]
["8.9","High",8937]
["8.99","High",15755]
["9.1","Low",8750]
["9.10","Medium",8759]
["9.11","Medium",8760]
["9.12","Medium",8761]
["9.13","Low",8762]
["9.14","Medium",8763]
["9.15","Medium",8764]
["9.16","High",8765]
["9.17","High",8766]
["9.18","Low",8767]
["9.19","Low",8768]
["9.2","Very High",8751]
["9.20","Medium",8769]
["9.21","Medium",8770]
["9.22","Low",8771]
["9.23","Low",8772]
["9.24","Medium",8773]
["9.25","Low",8774]
["9.26","Low",8775]
["9.27","Low",8776]
["9.28","Medium",8777]
["9.29","Low",8778]
["9.3","Very High",8752]
["9.4","High",8753]
["9.5","High",8754]
["9.6","Low",8755]
["9.7","Medium",8756]
["9.8","Medium",8757]
["9.9","Medium",8758]
["9.99","High",8779]

{"sheet":"Equipment_list","index":7,"n_rows":28,"n_cols":3,"rows_kept":28,"cut":false,"hidden":true,"merged":[]}
["TITLE","Equipment_list_description","ID"]
["Accommodation",null,12]
["Cargo Mach.",null,13]
["Critical Equip.",null,16]
["Deck - Machinery",null,18]
["Deck - Mooring Machinery",null,15]
["Deck - Pipe / Fittings",null,20]
["Documentation",null,21]
["E/R - Air Comp.",null,8]
["E/R - Aux. Engine",null,4]
["E/R - Aux. Mach.",null,7]
["E/R - Boiler",null,5]
["E/R - Main Engine",null,3]
["E/R - Pipes/ valves & fittings",null,9]
["E/R - Pumps",null,32]
["E/R - Purifier",null,6]
["Elect. Mach. & Equip.",null,10]
["Hull & Tanks",null,19]
["Inert Gas",null,14]
["LSA / FFA",null,17]
["Miscellaneous",null,22]
["Navigation - DGPS / EPFS / AIS",null,28]
["Navigation - ECDIS",null,25]
["Navigation - Echo Sounder / Speed Log",null,26]
["Navigation - GMDSS & Communication",null,23]
["Navigation - Others",null,11]
["Navigation - RADAR",null,24]
["Navigation - VDR / BNWAS",null,30]

{"sheet":"PSC_MOU","index":8,"n_rows":11,"n_cols":3,"rows_kept":11,"cut":false,"hidden":true,"merged":[]}
["TITLE","PSC_MOU_description","ID"]
["Asia and the Pacific",null,2]
["Caribbean",null,4]
["Europe and the North Atlantic",null,1]
["Latin America",null,3]
["The Black Sea region",null,6]
["The Indian Ocean",null,8]
["The Mediterranean",null,7]
["The Riyadh MoU",null,9]
["USCG",null,10]
["West and Central Africa",null,5]

{"sheet":"Inspection_type","index":9,"n_rows":13,"n_cols":2,"rows_kept":13,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Bunkering Audit",14]
["Cargo Audit",17]
["Engineering Audit",16]
["ISM Audit",2]
["ISPS Audit",3]
["IT Audit",10]
["MLC Audit",1]
["Mooring Audit",9]
["Nav Audit / Verification",8]
["Onboard Training",18]
["Ship Staff Insp.",15]
["Suptd. Insp.",13]

{"sheet":"Deficiency_Cause","index":10,"n_rows":8,"n_cols":3,"rows_kept":8,"cut":false,"hidden":true,"merged":[]}
["TITLE","Deficiency_Cause_description","ID"]
["Behaviour Based",null,1]
["Equipment Related",null,4]
["External Factors",null,5]
["Human Error",null,7]
["Inappropriate Procedure",null,8]
["Industry Issue",null,6]
["Knowledge Based",null,3]

{"sheet":"Observer_code","index":11,"n_rows":3,"n_cols":3,"rows_kept":3,"cut":false,"hidden":true,"merged":[]}
["TITLE","Observer_code_description","ID"]
["Owner / Marine / Tech. Suptd.",null,3]
["Ship Staff",null,2]

{"sheet":"Status_code","index":12,"n_rows":6,"n_cols":3,"rows_kept":6,"cut":false,"hidden":true,"merged":[]}
["TITLE","Status_code_description","ID"]
["Completed",null,6]
["Deferred to D D",null,5]
["In progress",null,3]
["Not Started",null,2]
["Waiting spare",null,4]

{"sheet":"PSC_ref_no","index":13,"n_rows":19,"n_cols":2,"rows_kept":19,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Alarms",9]
["Cargo operations including equipment",7]
["Certificates & Documentation",2]
["Dangerous Goods",13]
["Emergency Systems",5]
["Fire safety",8]
["ISM",16]
["ISPS",17]
["Life saving appliances",12]
["MLC, 2006",18]
["Other",19]
["Pollution Prevention",15]
["Propulsion and auxiliary machinery",14]
["Radio communication",6]
["Safety of Navigation",11]
["Structural condition",3]
["Water/Weathertight condition",4]
["Working and Living Conditions",10]

{"sheet":"Risk_value_of_obs","index":14,"n_rows":1,"n_cols":2,"rows_kept":1,"cut":false,"hidden":true,"merged":[]}
["Risk Value of observation","ID"]

{"sheet":"Year","index":15,"n_rows":18,"n_cols":1,"rows_kept":18,"cut":false,"hidden":true,"merged":[]}
["Year"]
[2014]
[2015]
[2016]
[2017]
[2018]
[2019]
[2020]
[2021]
[2022]
[2023]
[2024]
[2025]
[2026]
[2027]
[2028]
[2029]
[2030]

{"sheet":"Month","index":16,"n_rows":13,"n_cols":1,"rows_kept":13,"cut":false,"hidden":true,"merged":[]}
["Month"]
["Jan"]
["Feb"]
["Mar"]
["Apr"]
["May"]
["Jun"]
["Jul"]
["Aug"]
["Sep"]
["Oct"]
["Nov"]
["Dec"]

{"sheet":"Date_","index":17,"n_rows":32,"n_cols":1,"rows_kept":32,"cut":false,"hidden":true,"merged":[]}
["Date"]
["01"]
["02"]
["03"]
["04"]
["05"]
["06"]
["07"]
["08"]
["09"]
[10]
[11]
[12]
[13]
[14]
[15]
[16]
[17]
[18]
[19]
[20]
[21]
[22]
[23]
[24]
[25]
[26]
[27]
[28]
[29]
[30]
[31]

{"sheet":"Sheet1","index":18,"n_rows":24,"n_cols":6,"rows_kept":24,"cut":false,"hidden":true,"merged":[]}
[]
[null,"ID","E",null,"Date Recorded",1]
[null,"UNIQUE ID","F",null,"Type of Deficiency",2]
[1,"Date Recorded","G",null,"Observer code",3]
["ignore","Vessel Type","H",null,"Type of Inspection",4]
[null,"Internal / External","I",null,"Description of Deficiency",5]
[null,"Drydock","J",null,"Equipment Categories",6]
[null,"Information Sharing","K",null,"Area of Observation",7]
[null,"Critical_item","L",null,"Deficiency Cause",8]
[null,"Deficiency Type","M",null,"VIQ Ref Number",9]
[null,"Deficiency Cause","N",null,"Risk Value of Obs",10]
[null,"Inspection Type","O",null,"PSC Ref Number",11]
[null,"Equipments","P",null,"PSC MOU ID",12]
[null,"VIQ Reference Number","Q",null,"Action Taken or Required",13]
[null,"Risk Value of the observation","R",null,"Target Date",14]
[null,"PSC Reference Number","S",null,"PO Ref No.",15]
[null,"PSC MOU","T",null,"Status Code",16]
[null,"Observer Code","U",null,"Date Completed",17]
[null,"Target Date","V",null,"Drydock",18]
[null,"Status Code","W",null,"Info Sharing",19]
[null,"Description of Deficiency","X",null,"Critical Item Flag",20]
[null,"Action taken / required","Y",null,"Audit Type",21]
[null,"PO ref no","Z"]
[null,"Date completed","AA"]

{"sheet":"Ship_information","index":19,"n_rows":2,"n_cols":3,"rows_kept":2,"cut":false,"hidden":true,"merged":[]}
["Ship_ID","Ship_Name","FILE_NAME"]
["46","WAWASAN RUBY (29-04-2021)","46_1619685823256.xlsm"]

{"sheet":"External_Deficiency_type","index":20,"n_rows":5,"n_cols":3,"rows_kept":5,"cut":false,"hidden":true,"merged":[]}
["TITLE","Type of deficiency_description","ID"]
["Condn of Class / Memo",null,5]
["Defect",null,1]
["Non Conformity",null,2]
["Observation",null,3]

{"sheet":"External_Inspection_type","index":21,"n_rows":11,"n_cols":2,"rows_kept":11,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Cargo Audit",17]
["Flag State Insp.",5]
["ISM Audit",2]
["ISPS Audit",3]
["MLC Audit",1]
["Nav Audit / Verification",8]
["OM Insp. (Eg. SIRE / CDI etc.)",6]
["Others (Eg. Insurance etc.)",12]
["PSC Inspection",4]
["Terminal Insp.",11]

{"sheet":"External_Observer_code","index":22,"n_rows":7,"n_cols":3,"rows_kept":7,"cut":false,"hidden":true,"merged":[]}
["TITLE","Observer_code_description","ID"]
["Class Surveyor",null,4]
["FSC Inspector",null,5]
["Others (Eg. Insurance etc.)",null,9]
["PSC Insp.",null,6]
["SIRE / CDI Insp.",null,8]
["Terminal Insp.",null,7]

{"sheet":"Sheet Version","index":23,"n_rows":2,"n_cols":2,"rows_kept":2,"cut":false,"hidden":true,"merged":[]}
["Version","Title"]
["2.0","Version 2.0"]