{"text_format":"1","workbook":"xlsx","n_sheets":24,"sheets":["Mainsheet","Completed","Calc","Areaofobs","Vessel_type","Deficiency_type","VIQrefno","Equipment_list","PSC_MOU","Inspection_type","Deficiency_Cause","Observer_code","Status_code","PSC_ref_no","Risk_value_of_obs","Year","Month","Date_","Sheet1","Ship_information","External_Deficiency_type","External_Inspection_type","External_Observer_code","Sheet Version"],"not_rendered":{"charts":0,"images":5,"macros":1,"external_links":0,"defined_names":12,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Mainsheet","index":0,"n_rows":79,"n_cols":28,"rows_kept":79,"cut":false,"hidden":false,"merged":[[10,8,10,9],[10,12,10,13],[12,6,12,27],[8,6,8,27]]}
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,"Defect - Damage Monitoring Sheet"]
[]
[null,null,null,null,null,null,null,"Date of Report","16-Mar-2021",null,null,"Ship Name","ZENO (16-03-2021)"]
[]
[null,null,null,null,null,null,"VERSION : 2.0"]
[]
[]
[]
[null,null,null,null,"ID","UNIQUE ID","Date Recorded","Type of Deficiency","Observer code","Type of Inspection","Description of Deficiency","Equipment Categories","Area of Observation","Deficiency Cause","VIQ Ref Number","Risk Value of Obs","PSC Ref Number","PSC MOU ID","Action Taken or Required","Target Date","PO Ref No.","Status Code","Date Completed","Drydock","Info Sharing","Critical Item","Audit Type","Superintendent Remarks"]
[null,null,null,null,16810,"36_5/1/2021 1:38:20 PM","2020-10-28","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Funnel deck to be chipped and painted.","Miscellaneous","General Appearance","Equipment Related",11.8,"Low","Not Applicable","Not Applicable","On the Funnel Deck, there are Soft Patches at Various locations and also thick rust. Job included in DD.","2021-09-30",null,"Deferred to D D",null,"No","No","No","Internal"]
[null,null,null,null,null,"36_22/3/2021 10:05:18 AM","2020-01-30","Defect","Ship Staff","Ship Staff Insp.","Mooring Winch Forecastle W1 (Stbd Side Outer) Bush Bearing Broken.","Deck - Mooring Machinery","Mooring","Equipment Related",9.14,"Medium","Not Applicable","Not Applicable","Bush bearing to be renewed. Included in Ref Man. Dry Dock Job.","2021-09-30","ZENO200016","Deferred to D D",null,"Yes",null,null,"Internal"]
[null,null,null,null,null,"36_22/3/2021 10:16:51 AM","2020-04-04","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Windlass Stbd Side W1 rope drum bearing is damaged. Vessel has to check the condition of the other bearings on Stbd Windlass and amend the orders accordingly.","Deck - Mooring Machinery","Mooring","Equipment Related",9.1999999999999993,"Very High","Not Applicable","Not Applicable","Included in Refman for rectification during the next dry docking.","2021-09-30","ZENO200016","Deferred to D D",null,"No",null,null,"Internal"]
[null,null,null,null,null,"36_21/3/2021 7:34:20 PM","2020-08-22","Critical Equipment","Ship Staff","Ship Staff Insp.","Port Anchor: Observed Stud Missing on the Common Link after the 5th Kenter Shackle.","Deck - Mooring Machinery","Mooring","Equipment Related",9.1999999999999993,"Very High","Not Applicable","Not Applicable","Anchor chain common link (Stud) received at Lome 29-May-2021.Job included in DD.","2021-09-30",null,"Deferred to D D",null,"No",null,null,"Internal"]
[null,null,null,null,null,"36_21/3/2021 7:27:45 PM","2020-08-26","Observation","Ship Staff","Ship Staff Insp.","All Winches Leaking from the operating Blocks handles.","Deck - Mooring Machinery","Mooring","Equipment Related",9.14,"Medium","Not Applicable","Not Applicable","Spares received. Job to be started.\r\n","2021-08-31",null,"In progress",null,"No",null,null,"Internal"]
[null,null,null,null,16811,"36_6 Jan 2021 12:12:30 PM","2020-10-28","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Fresh Water Generator No. 2 Jacket water valves are not holding. To be renewed and FWG Cleaned.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","FWG plates are being cleaned with chemical circulation. Need to do black out to carryout the job. ","2021-08-15",null,"Deferred to D D",null,"No","No","No","Internal"]
[null,null,null,null,16812,"36_6 Jan 2021 12:22:08 PM","2020-10-28","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Bottom plate of the Hot well is corroded in some sections. \n\nTo be repaired at a suitable opportunity. The top of hot well tank is to be cleaned properly and painted. \n\n","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","\n\nTo be repaired at a suitable opportunity. The top of hot well tank is cleaned and painted. \n\n","2021-08-15",null,"Deferred to D D",null,"No","No","No","Internal"]
[null,null,null,null,16813,"36_6 Jan 2021 12:25:41 PM","2020-10-28","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Two flanges on Aux CSW pump discharge line found leaking. One going to COP line and another to LT Cooler. Gaskets to be renewed.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Need to do black out to carry out the job. waiting for suitable oppertunity.","2021-08-15",null,"Deferred to D D",null,"No","No","No","Internal"]
[null,null,null,null,16815,"36_6 Jan 2021 12:41:35 PM","2020-10-28","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Stbd Aux. Boiler uptake found holed. To be included in Refman for rectification during the next docking related repairs.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","To be included in Refman for rectification during the next docking related repairs.","2021-06-30","","Deferred to D D",null,"Yes","No","No","Internal"]
[null,null,null,null,16817,"36_6/1/2021 2:49:09 PM","2020-10-28","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","The steam lines for the deck seal to be de-rusted and painted.","E/R - Pipes/ valves & fittings","Cargo / Ballast Systems","Equipment Related",8.15,"High","Not Applicable","Not Applicable","Derusting and painting of the steam lines to carried out.","2021-08-31",null,"Not Started",null,"No","No","No","Internal"]
[null,null,null,null,16821,"36_6/1/2021 3:16:15 PM","2020-10-28","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Both crane winches to be de rusted and painted.","Deck - Machinery","General Appearance","Equipment Related",8.5,"Very High","Not Applicable","Not Applicable","Crane winches to be derusted and painted.","2021-08-31",null,"Not Started",null,"No","No","No","Internal"]
[null,null,null,null,16822,"36_6/1/2021 3:19:37 PM","2020-10-28","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Emergency hand pump hatch cover for both the cranes is in poor condition. The hatch cover lips to be repaired.","Deck - Machinery","General Appearance","Equipment Related",8.5,"Very High","Not Applicable","Not Applicable","The hatch cover lips to be repaired. Job included in Refman DD specs.","2021-09-30",null,"Deferred to D D",null,"No","No","No","Internal"]
[null,null,null,null,16823,"36_6/1/2021 3:22:48 PM","2020-10-28","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Main Deck port side from gangway till the break of accommodation and from 1 port to mid-ship area to be spot chipped and painted.","Deck - Pipe / Fittings","General Appearance","Equipment Related",11.3,"Medium","Not Applicable","Not Applicable","Maintenance on deck is affected due to continuous back to back STS operation, and also vessel does not have hydro blaster. Maintenance is in progress as vessel gets opportunity when there is no STS operation.","2021-08-31",null,"In progress",null,"No","No","No","Internal"]
[null,null,null,null,16824,"36_6/1/2021 3:25:44 PM","2020-10-28","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Monkey island to be spot chipped and painted. Christmas tree light foundations and brackets are to be renewed. ","Accommodation","General Appearance","Equipment Related",11.8,"Low","Not Applicable","Not Applicable","Derusting and painting to be carried out. Christmas tree light foundations and brackets are to be renewed. ","2021-08-31",null,"Not Started",null,"No","No","No","Internal"]
[null,null,null,null,16825,"36_6/1/2021 3:28:58 PM","2020-10-28","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Flanges and bolts of pipelines on main deck to be chipped and painted.","Deck - Pipe / Fittings","General Appearance","Equipment Related",11.4,"Very High","Not Applicable","Not Applicable","Derusting and painting to be carried out.","2021-08-31",null,"In progress",null,"No","No","No","Internal"]
[null,null,null,null,null,"36_22/3/2021 10:37:19 AM","2020-10-28","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","VECS O2 Sensor failed. Last renewed May 2019 (17 mnths Old, as per maker to be replaced every 12 mnths). Filter is completely Choked, giving Low Flow alarm.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related",8.33,"Medium","Not Applicable","Not Applicable","Filter was cleaned on board, managed only 40-50% clean, fixed back, Low Flow alaram gone. But it can Clog any time. Low Flow Alarm may come again. Recieved  filter & O2 Sensor.Requisition raised for power supply unit.","2021-08-15","ZENO210124","Waiting spare",null,"No",null,null,"Internal"]
[null,null,null,null,null,"36_22/3/2021 10:44:33 AM","2020-10-28","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Swivel for Stbd anchor clearance is high. Same to be included in refman for rectification during the next docking related repairs.","Deck - Mooring Machinery","Mooring","Equipment Related",9.1999999999999993,"Very High","Not Applicable","Not Applicable","Included in Refman for rectification during the dry dock.","2021-09-30",null,"Deferred to D D",null,"No",null,null,"Internal"]
[null,null,null,null,null,"36_22/3/2021 10:49:13 AM","2020-10-28","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Mooring Windlass brake drum heavily corroded. to be derusted. Same to be included in refman for rectification during the next docking related repairs.","Deck - Mooring Machinery","Mooring","Equipment Related",9.1999999999999993,"Very High","Not Applicable","Not Applicable","Included in refman for rectification during the dry dock.","2021-09-30",null,"Deferred to D D",null,"No",null,null,"Internal"]
[null,null,null,null,null,"36_22/3/2021 11:28:51 AM","2021-02-25","Observation","Ship Staff","Ship Staff Insp.","Abnormal Sound while operating forward W2 Winch.","Deck - Mooring Machinery","Mooring","Equipment Related",9.14,"Medium","Not Applicable","Not Applicable","Presently Vessel is engaged in continuous back to back STS  cargo operations & Port windlass is always in use, due to STS vessel on stbd side and the job can not be planned here during STS operation, same is deffered for DD.","2021-09-30",null,"Deferred to D D",null,"No",null,null,"Internal"]
[null,null,null,null,null,"36_22/3/2021 11:38:03 AM","2021-02-25","Observation","Ship Staff","Ship Staff Insp.","Cargo tanks heating coil are not provided with drip tray.","Deck - Pipe / Fittings","MARPOL Related","Equipment Related,Industry Issue",8.15,"High","Not Applicable","Not Applicable","Included in refman Dry Dock Jobs.","2021-09-30",null,"Deferred to D D",null,"No",null,null,"Internal"]
[null,null,null,null,null,"36_22/3/2021 2:02:44 PM","2021-02-25","Defect","Ship Staff","Ship Staff Insp.","The tank pressure reading of 6S COT is slightly erratic.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related",8.25,"Very High","Not Applicable","Not Applicable","ZENO210057 - Cargo Tank Pressure Monitoring System - Vapour Pressure Sensor requisition raised.","2021-09-30","ZENO21005","Waiting spare",null,"No",null,null,"Internal"]
[null,null,null,null,null,"36_22/3/2021 2:09:05 PM","2021-02-25","Observation","Ship Staff","Ship Staff Insp.","Foam Monitor on Deck leaking from bearing.","LSA / FFA","Safety / LSA / FFA","Equipment Related",5.35,"Medium","Not Applicable","Not Applicable","Inspection of  Foam Monitors carried out Groovings noted inside of bearing Assembly  & O rings Grooving too deep and unable to provide proper sealing causing leaks. ZENO210102 - FOAM MONITOR BEARING SET requisition Raised.","2021-09-30","ZENO210102","Waiting spare",null,"No",null,null,"Internal"]
[null,null,null,null,null,"36_22/3/2021 2:20:40 PM","2021-02-25","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Pressure side & Vaccum side of Spare PV valve defective.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related",8.4,"High","Not Applicable","Not Applicable","ZENO210042 - High Velocity pressure Vaccum Valve requisition raised.","2021-05-25","ZENO210042","Waiting spare",null,"No",null,null,"Internal"]
[null,null,null,null,null,"36_22/3/2021 2:28:01 PM","2021-02-25","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Stbd side Manifold stand between No1 and No2 & No.2 and No.3 holed.","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","Equipment Related",11.8,"Low","Not Applicable","Not Applicable","Job included in Refman for Dry Docking Repairs.","2021-09-30",null,"Deferred to D D",null,"No",null,null,"Internal"]
[null,null,null,null,null,"36_22/3/2021 2:41:36 PM","2021-02-25","Observation","Ship Staff","Ship Staff Insp.","Vessel does not have spare Pilot Ladder.","Miscellaneous","Safety / LSA / FFA","External Factors",5.27,"Medium","Not Applicable","Not Applicable","RO raised - RO ZENO210098 / Awaiting supply","2021-09-30","RO ZENO210098 ","Waiting spare",null,"No",null,null,"Internal"]
[null,null,null,null,null,"36_22/3/2021 2:44:34 PM","2021-02-25","Observation","Ship Staff","Ship Staff Insp.","Vessel does not have spare provision crane wire.","Deck - Machinery","Cargo / Ballast Systems","Equipment Related",8.5,"Very High","Not Applicable","Not Applicable","RO raised - RO  ZENO210028 / Awaiting supply","2021-09-30","-RO  ZENO210028 ","Waiting spare",null,"No",null,null,"Internal"]
[null,null,null,null,null,"36_22/3/2021 2:48:17 PM","2021-02-25","Observation","Ship Staff","Ship Staff Insp.","Vessel does not have spare gangway & Lifeboat Wire.","LSA / FFA","Safety / LSA / FFA","Equipment Related",5.27,"Medium","Not Applicable","Not Applicable","RO raised - RO  ZENO210028 / Awaiting supply","2021-09-30","RO  ZENO210028 ","Waiting spare",null,"No",null,null,"Internal"]
[null,null,null,null,null,"36_22/3/2021 2:51:20 PM","2021-02-25","Non Conformity","Ship Staff","Ship Staff Insp.","Deratting Certificate Expired.","Documentation","Cert. & Docu.","External Factors",2.1,null,"Not Applicable","Not Applicable","Same will be arranged at Lome by Ops Dept.","2021-05-25",null,"In progress",null,"No",null,null,"Internal"]
[null,null,null,null,null,"36_26/3/2021 9:12:22 AM","2021-02-25","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Funnel deck soft patches.","Hull & Tanks","Structural Condn. / WT integrity ","External Factors",11.8,"Low","Not Applicable","Not Applicable","Job included in refman for dry docking related reapirs.","2021-09-30",null,"Deferred to D D",null,"No",null,null,"Internal"]
[null,null,null,null,null,"36_26/3/2021 9:19:36 AM","2021-02-25","Observation","Ship Staff","Ship Staff Insp.","Storage fridge for foodwaste is not working","Miscellaneous","MLC Related","Equipment Related",6.2,"High","Not Applicable","Not Applicable","Fridge is not cooling and cannot be rectified onboard.Inspection carried out by ETO. Requisition Raised. ZENO210083 , awaiting supply.","2021-09-30"," ZENO210083 ","Waiting spare",null,"No",null,null,"Internal"]
[null,null,null,null,null,"36_26/3/2021 9:30:07 AM","2021-02-25","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Metal frames of Tank Heating Coils Manifolds on deck were found rusty with holes. ","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related",11.8,"Low","Not Applicable","Not Applicable","Job  included in Refman for forthcoming DD.","2021-09-30",null,"Deferred to D D",null,"No",null,null,"Internal"]
[null,null,null,null,null,"36_26/3/2021 9:35:04 AM","2021-02-25","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Safety catwalks on deck were found rusty and edge plates were missing","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","Equipment Related",11.8,"Low","Not Applicable","Not Applicable","Job included in refman for Dry Docking related repairs.","2021-09-30",null,"Deferred to D D",null,"No",null,null,"Internal"]
[null,null,null,null,null,"36_28/3/2021 4:22:56 PM","2021-02-25","Defect","Ship Staff","Ship Staff Insp.","No. 1 GMDSS Walkie Talkie Screen Faulty.","Navigation - Others","Navigation","Equipment Related",4.2699999999999996,"High","Not Applicable","Not Applicable","Requistion ZENO210038 raised.","2021-05-25","ZENO210038","Waiting spare",null,"No",null,null,"Internal"]
[null,null,null,null,null,"36_13 Jun 2021 11:19:03 AM","2021-03-05","Defect","Ship Staff","Ship Staff Insp.","COT 6 S pressure sensor showing 30mmWG more","Cargo Mach.","Cargo / Ballast Systems","Equipment Related",8.19,null,"Not Applicable","Not Applicable","Need to replace pressure sensor","2021-08-15","zeno 210057","Waiting spare",null,"No",null,null,"Internal"]
[null,null,null,null,null,"36_28/3/2021 3:05:53 PM","2021-03-28","Defect","Ship Staff","Ship Staff Insp.","Main engine exhaust remote temperature of unit no 5 and 6 is showing more than local temperature, hence exhaust gas temperature is more","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Main engine thermocouple amplifier to be renewed.","2021-07-30","ZENO210002","In progress",null,"No",null,null,"Internal"]
[null,null,null,null,null,"36_28/3/2021 3:16:39 PM","2021-03-28","Defect","Ship Staff","Ship Staff Insp.","Some IG panel indication lights in ECR and CCR are not working","Inert Gas","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Indication lights to be renewed.","2021-05-30","ZENO210022","Waiting spare",null,"No",null,null,"Internal"]
[null,null,null,null,null,"36_28/3/2021 3:29:30 PM","2021-03-28","Defect","Ship Staff","Ship Staff Insp.","Two numbers of search light reflector on bridge wing are not in good condition.","Navigation - Others","Navigation","Equipment Related",4.8,"Medium","Not Applicable","Not Applicable","Search light reflector to be renewed. on 28th May 2021 only one reflector was recieved in the store, same installed on STBD side search light, awaiting supply of one more reflector to complete the job. ","2021-05-30","ZENO210041","Waiting spare",null,"No",null,null,"Internal"]
[null,null,null,null,null,"36_28/3/2021 3:51:23 PM","2021-03-28","Observation","Ship Staff","Ship Staff Insp.","No high level alarm fitted in cascade tank","Miscellaneous","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","High level alarm to be fitted in drydock","2021-08-15",null,"Deferred to D D",null,"Yes",null,null,"Internal"]
[null,null,null,null,null,"36_28/3/2021 3:53:49 PM","2021-03-28","Defect","Ship Staff","Ship Staff Insp.","Cascade tank body corroded on port side","Miscellaneous","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","To be repaired in drydock","2021-08-15",null,"Deferred to D D",null,"Yes",null,null,"Internal"]
[null,null,null,null,null,"36_28/3/2021 3:57:11 PM","2021-03-28","Defect","Ship Staff","Ship Staff Insp.","Control air compressor inoperational","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Bearings to be renewed","2021-08-15","Requisition raised by owners","Waiting spare",null,"No",null,null,"Internal"]
[null,null,null,null,null,"36_28 Mar 2021 5:14:45 PM","2021-03-28","Defect","Ship Staff","Ship Staff Insp.","Galley fan control unit inoperational","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Solenoid valve to be renewed.","2021-05-30","ZENO210072","Waiting spare",null,"No",null,null,"Internal"]
[null,null,null,null,null,"36_28 Mar 2021 5:21:59 PM","2021-03-28","Defect","Ship Staff","Ship Staff Insp.","Aux boiler number 1 smoke density is not showing reading.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Potentiometer to be renewed.","2021-05-30","ZENO210070","Waiting spare",null,"No",null,null,"Internal"]
[null,null,null,null,null,"36_28 Mar 2021 5:35:57 PM","2021-03-28","Defect","Ship Staff","Ship Staff Insp.","Fresh water generator no 2 jacket water inlet and outlet valves are not holding.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Jacket water inlet and outlet valve to be renewed.","2021-08-15",null,"Deferred to D D",null,"No",null,null,"Internal"]
[null,null,null,null,null,"36_30/3/2021 10:53:04 AM","2021-03-30","Defect","Ship Staff","Ship Staff Insp.","Fire and GS pump discharge valves and overboard valve are not holding.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Fire and GS pump discharge valves and overboard valve to be renewed in drydock.","2021-08-15",null,"Deferred to D D",null,"No",null,null,"Internal"]
[null,null,null,null,null,"36_30/3/2021 10:59:54 AM","2021-03-30","Defect","Ship Staff","Ship Staff Insp.","ME jacket pre heater3 tubes are plugged","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","ME jacket pre heatertubes to be renewed.","2021-08-15",null,"Deferred to D D",null,"No",null,null,"Internal"]
[null,null,null,null,null,"36_30/3/2021 11:05:20 AM","2021-03-30","Defect","Ship Staff","Ship Staff Insp.","Sludge pump suction line to oily bilge tank is choked.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Sludge pump suction line to oily bilge tank is choked.","2021-05-30",null,"Not Started",null,"No",null,null,"Internal"]
[null,null,null,null,null,"36_30/3/2021 3:46:55 PM","2021-03-30","Defect","Ship Staff","Ship Staff Insp.","Aux boiler steam warm up valves are not holding.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Aux boiler steam warm up valves to be overhauled.","2021-05-30",null,"Not Started",null,"No",null,null,"Internal"]
[null,null,null,null,null,"36_30/3/2021 4:16:13 PM","2021-03-30","Defect","Ship Staff","Ship Staff Insp.","Aux boiler FO supply pump 3 way valve not holding.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Aux boiler FO supply pump 3 way valve to be ovarhaulled.","2021-08-15","ZENO200101","Deferred to D D",null,"No",null,null,"Internal"]
[null,null,null,null,null,"36_30/3/2021 4:30:39 PM","2021-03-30","Defect","Ship Staff","Ship Staff Insp.","Emergency fire pump Q-vac system inoperational.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Q-vac system to be overhauled.","2021-05-30","ZENO210015","Waiting spare",null,"No",null,null,"Internal"]
[null,null,null,null,null,"36_30/3/2021 4:44:52 PM","2021-03-30","Defect","Ship Staff","Ship Staff Insp.","Incinerator refractory is damage.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Refractory to be repaired.","2021-08-15","ZENO210050","Deferred to D D",null,"No",null,null,"Internal"]
[null,null,null,null,null,"36_30/3/2021 4:47:53 PM","2021-03-30","Defect","Ship Staff","Ship Staff Insp.","Aux boiler no 1 heating coil is leaking.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Heating coil to be repaired in drydock.","2021-08-15",null,"Deferred to D D",null,"Yes",null,null,"Internal"]
[null,null,null,null,null,"36_30/3/2021 4:55:51 PM","2021-03-30","Defect","Ship Staff","Ship Staff Insp.","Hole in the soot tank drain line.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Soot tank drain line to be repaired by hotwork.","2021-08-15",null,"Deferred to D D",null,"No",null,null,"Internal"]
[null,null,null,null,null,"36_30/3/2021 5:00:25 PM","2021-03-30","Defect","Ship Staff","Ship Staff Insp.","Aux boiler water feed pump inoperational.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Aux boiler water feed pump to be overhauled.","2021-08-15","ZENO210044","Waiting spare",null,"No",null,null,"Internal"]
[null,null,null,null,null,"36_30/3/2021 5:06:13 PM","2021-03-30","Defect","Ship Staff","Ship Staff Insp.","Expansion tank level guage spring loaded valve is leaking when pressed.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Gland packings/bushing to be renewed.","2021-08-15",null,"Not Started",null,"No",null,null,"Internal"]
[null,null,null,null,null,"36_30/3/2021 5:23:01 PM","2021-03-30","Defect","Ship Staff","Ship Staff Insp.","Various insulation laggings in engine room needs to be repaired.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related",11.5,"Medium","Not Applicable","Not Applicable","Various insulation laggings in engine room needs to be repaired.","2021-05-30","Included in engine room stores ZENO210050","In progress",null,"No",null,null,"Internal"]
[null,null,null,null,null,"36_30/3/2021 5:29:40 PM","2021-03-30","Defect","Ship Staff","Ship Staff Insp.","Fire and GS pump discharge line got holed.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","To be repaired by hotwork.","2021-08-15",null,"Deferred to D D",null,"No",null,null,"Internal"]
[null,null,null,null,null,"36_31/3/2021 8:59:11 AM","2021-03-31","Defect","Ship Staff","Ship Staff Insp.","Stern tube forward seal is leaking","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Job to be carried out in drydock","2021-08-15",null,"Deferred to D D",null,"Yes",null,null,"Internal"]
[null,null,null,null,null,"36_13 Jun 2021 10:40:27 AM","2021-04-21","Breakdown","Ship Staff","Ship Staff Insp.","Main lube oil pump no. 1 is inoperational","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Pump to be overhauled. Bearings, oil seal, bearing collor and upper shaft to be renewed.","2021-08-15","ZENO210096","Waiting spare",null,"No",null,null,"Internal"]
[null,null,null,null,null,"36_15/6/2021 3:09:32 PM","2021-05-20","Defect","Ship Staff","Ship Staff Insp.","SAAB Rosemount PC, COT 1S  not showing any readings - TGE Faulty.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related",8.4,"High","Not Applicable","Not Applicable","Troubleshooting is in progress with Office.","2021-08-20",null,"In progress",null,"No",null,null,"Internal"]
[null,null,null,null,null,"36_13 Jun 2021 11:24:49 AM","2021-06-03","Defect","Ship Staff","Ship Staff Insp.","Tank Overfill alarm power supply not in operational ","Cargo Mach.","Cargo / Ballast Systems","Equipment Related",8.19,null,"Not Applicable","Not Applicable","Need to replace","2021-08-15","ZENO210110","Waiting spare",null,"No",null,null,"Internal"]
[null,null,null,null,null,"36_13 Jun 2021 11:27:41 AM","2021-06-11","Defect","Ship Staff","Ship Staff Insp.","A/E # 1 T/C outlet temp sensor faulty\t\t","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","need to replace","2021-08-15","ZENO210119","Waiting spare",null,"No",null,null,"Internal"]
[null,null,null,null,null,"36_13 Jun 2021 11:31:00 AM","2021-06-12","Defect","Ship Staff","Ship Staff Insp.","VECS power supply not in operational","Cargo Mach.","Cargo / Ballast Systems","Equipment Related",8.19,null,"Not Applicable","Not Applicable","Need to replace","2021-08-15","ZENO210124","Waiting spare",null,"No",null,null,"Internal"]

{"sheet":"Completed","index":1,"n_rows":242,"n_cols":28,"rows_kept":242,"cut":false,"hidden":false,"merged":[[10,8,10,9],[10,12,10,13],[12,6,12,27],[8,6,8,27]]}
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,"Defect - Damage Monitoring Sheet"]
[]
[null,null,null,null,null,null,null,"Date of Report","16-Mar-2021",null,null,"Ship Name","ZENO (16-03-2021)"]
[]
[null,null,null,null,null,null,"VERSION : 2.0"]
[]
[]
[]
[null,null,null,null,"ID","UNIQUE ID","Date Recorded","Type of Deficiency","Observer code","Type of Inspection","Description of Deficiency","Equipment Categories","Area of Observation","Deficiency Cause","VIQ Ref Number","Risk Value of Obs","PSC Ref Number","PSC MOU ID","Action Taken or Required","Target Date","PO Ref No.","Status Code","Date Completed","Drydock","Info Sharing","Critical Item","Audit Type","Superintendent Remarks"]
[null,null,null,null,2795,"36_13/10/2019 4:18:50 PM","2019-01-08","Defect","Ship Staff","Ship Staff Insp.","Signal column light for E/R workshop and outside E/R workshop audible alarm found not working","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.21","Medium","","","same been renewed with spare recieved","2019-05-31","ZENO190025","Completed","2019-05-18","No","No","No","Internal"]
[null,null,null,null,8193,"36_Thu Dec 05 2019 03:35:54 GMT+0000 (Coordinated Universal Time)","2019-01-29","Defect","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","The rated working pressure as per cargo lines plan was 14.9 kg/cm2 however, the lines were pressure tested only at 14.9 kg/cm2 on 04 July 2018 during previous docking to 1.5 times of its MAWP instead of 22.35 kg/cm2.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Inappropriate Procedure","8.3","Very High","","","Cargo lines was pressure tested to 16 kg/cm2 in dry dock.Vessel Had already changed the maximum working pressure to 10.5 kg/cm2 which is in compliance with the tested pressure in drydock.","2021-06-30","","Completed","2019-01-29","Yes","No","No","External"]
[null,null,null,null,8178,"36_Sun May 12 2019 03:42:12 GMT+0000 (Coordinated Universal Time)","2019-01-29","Defect","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","Both the manifold pressure gauges glass (to which loading arms were connected) were crack.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.41","Medium","","","Manifold pressure gauges were renewed. ","2019-02-05","","Completed","2019-02-02","No","No","No","External"]
[null,null,null,null,8179,"36_Sun May 12 2019 03:52:32 GMT+0000 (Coordinated Universal Time)","2019-01-29","Defect","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","It was observed that flukes for port anchor did not make contact with the hull when the anchor was housed and chain stopper was in place.","Deck - Mooring Machinery","Mooring","Human Error","9.2","Very High","","","Anchor Heaved up and housed properly","2019-02-01","","Completed","2019-01-29","No","No","No","External"]
[null,null,null,null,8971,"36_Sun Oct 13 2019 13:17:55 GMT+0000 (Coordinated Universal Time)","2019-01-31","Defect","Ship Staff","Ship Staff Insp.","Fire,bilge and GS pp #1 found leaking from the mechanical seal\t","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.35","Medium","","","renewed with the spare ","2019-02-10","","Completed","2019-02-10","No","No","No","Internal"]
[null,null,null,null,11393,"36_14 Feb 2020 2:22:01 AM","2019-01-31","Defect","Ship Staff","Engineering Audit","Control air dryer is working with less efficiency. Dryer used to trip frequently due to high discharge pressure.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Gas charge reduced. Requisiton raised for a new dryer assembly.Spare received.Gas charged in the syatem.Working satisfactory.","2020-06-30","ZENO190053","Completed","2020-06-20","No","No","No","Internal"]
[null,null,null,null,2793,"36_2019-10-13 13:17:55.000","2019-01-31","Defect","Ship Staff","Ship Staff Insp.","Fire,bilge and GS pp #1 found leaking from the mechanical seal\t","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","renewed with the spare ","2019-02-10","","Completed","2019-02-10","No","No","No","Internal"]
[null,null,null,null,2800,"36_13/10/2019 4:37:51 PM","2019-02-01","Defect","Ship Staff","Ship Staff Insp.","IG o2 analyser # 1 faulty","Inert Gas","Eng. / Strg. Comp.","Equipment Related","8.26","High","","","same been repared with spare","2019-05-31","ZENO190051","Completed","2019-05-18","No","No","No","Internal"]
[null,null,null,null,2794,"36_13/10/2019 1:24:25 PM","2019-02-10","Defect","Ship Staff","Ship Staff Insp.","VRCS unit pressure switch malfunctioning\t","Deck - Machinery","Cargo / Ballast Systems","Equipment Related","8.18","High","","","same been renewed with the spare","2019-03-20","","Completed","2019-02-20","No","No","No","Internal"]
[null,null,null,null,2796,"36_13/10/2019 4:22:47 PM","2019-02-12","Defect","Ship Staff","Ship Staff Insp.","AC compressor # 1 L.O pressure regulating valve found leaking ","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","same been renewed with the spare recieved ","2019-05-31","ZENO190119","Completed","2019-05-20","No","No","No","Internal"]
[null,null,null,null,2801,"36_13/10/2019 4:41:30 PM","2019-02-28","Defect","Ship Staff","Ship Staff Insp.","VECS system oxygen sensor expired","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.25","Very High","","","same been renewed with spare one","2019-05-31","ZENO190101","Completed","2019-05-20","No","No","No","Internal"]
[null,null,null,null,2813,"36_13/10/2019 6:52:51 PM","2019-02-28","Defect","Ship Staff","Ship Staff Insp.","Pilot ladder magnets cracked and broken into pieces","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.47","Medium","","","magnets been renewed ","2019-07-31","ZENO190103","Completed","2019-07-31","No","No","No","Internal"]
[null,null,null,null,2797,"36_13/10/2019 4:26:36 PM","2019-03-01","Defect","Ship Staff","Ship Staff Insp.","IGS deck seal line flow control amplifier malfunctioning","Elect. Mach. & Equip.","Cargo / Ballast Systems","Equipment Related","8.26","High","","","same been renewed with spare recieved ","2019-05-31","ZENO190112","Completed","2019-05-19","No","No","No","Internal"]
[null,null,null,null,2806,"36_13/10/2019 5:04:19 PM","2019-03-12","Defect","Ship Staff","Ship Staff Insp.","One VHF (P) working only on low frequency range, same been observed from take over","Navigation - GMDSS & Communication","Communication","Equipment Related","","","","","working satisfactory","2019-03-31","","Completed","2019-05-18","No","No","No","Internal"]
[null,null,null,null,2799,"36_13/10/2019 4:34:46 PM","2019-03-15","Breakdown","Ship Staff","Ship Staff Insp.","FBB unit found not operational","Elect. Mach. & Equip.","Communication","Equipment Related","","","","","Fault finding done as per the email from the office ","2019-05-31","","Completed","2019-05-25","No","No","No","Internal"]
[null,null,null,null,8180,"36_Thu Dec 05 2019 04:06:26 GMT+0000 (Coordinated Universal Time)","2019-03-24","Defect","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","The port pilot ladder in use had side ropeswith joints just above last bottom stepwhich was not in compliance with resolution a.1045(27)pilot transfer arrangements 2.2.1 (The side ropes of the pilot ladder should consist of two unconverted ropesnot lessthan 18mm in diameter on each side and should be continuous, with no joints)","Deck - Machinery","Mooring","Inappropriate Procedure","5.47","Medium","","","Side ropes replaced with the spare ropes on board","2019-04-04","","Completed","2019-03-24","No","No","No","External"]
[null,null,null,null,2805,"36_13/10/2019 4:59:48 PM","2019-03-25","Defect","Owner / Marine / Tech. Suptd.","Ship Staff Insp.","No caliberation gases for portable gas meter","Critical Equip.","Cargo / Ballast Systems","Industry Issue","8.34","High","","","same been supplied","2019-05-31","","Completed","2019-05-18","No","No","No","External"]
[null,null,null,null,2798,"36_13/10/2019 4:29:53 PM","2019-03-28","Defect","Ship Staff","Ship Staff Insp.","Two foam monitor on the deck found leaking from the sleeves","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.35","Medium","","","same been renewed with thspare recieved","2019-05-31","ZENO190114","Completed","2019-05-20","No","No","No","Internal"]
[null,null,null,null,2783,"36_14/10/2019 12:13:14 AM","2019-03-29","Defect","Ship Staff","Ship Staff Insp.","ME alpha lubricator BCU unit PCB malfunctioning for stop singal from ME governor Elect.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Spare PCB received. Shore technician rectified the trouble without reneweing the PCB. ","2019-10-15","ZENO190128","Completed","2019-09-09","No","No","No","Internal","Ordered items supplied at Singapore on 08/10/2019.\nPls revert with updated status for PCB renewal."]
[null,null,null,null,2811,"36_13/10/2019 6:39:51 PM","2019-04-04","Breakdown","Ship Staff","Ship Staff Insp.","A/B main feed pp # 2 motor winding low insulation came and later found out winding damaged","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","motor been renewed with spare recieved","2019-07-31","ZENO1901952","Completed","2019-07-31","No","No","No","Internal"]
[null,null,null,null,2818,"36_13/10/2019 7:16:38 PM","2019-04-11","Defect","Ship Staff","Ship Staff Insp.","ACONIS station #3 DI 16 CARD # 7 in error condition ","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","same been renewed with spare one ","2019-07-31","ZENO195039","Completed","2019-07-23","No","No","No","Internal"]
[null,null,null,null,2825,"36_13/10/2019 11:07:37 PM","2019-04-16","Defect","Ship Staff","Ship Staff Insp.","VRCS system aux relay for pump cut in/cut out found malfunctioning","Elect. Mach. & Equip.","Cargo / Ballast Systems","Equipment Related","8.18","High","","","same been renewed with new one recieved ","2019-07-31","ZENO190089","Completed","2019-08-05","No","No","No","Internal"]
[null,null,null,null,2822,"36_13/10/2019 9:23:39 PM","2019-04-30","Defect","Ship Staff","Ship Staff Insp.","AE#3 exhaust outlet sensor found malfunctioning","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","8.13","Medium","","","same been renewed with new one","2019-07-31","ZENO19007","Completed","2019-07-25","No","No","No","Internal"]
[null,null,null,null,2826,"36_13/10/2019 11:23:25 PM","2019-04-30","Defect","Ship Staff","Ship Staff Insp.","AE #2 priming pump mechanical seal leaking","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","same seal been renewed with new one","2019-07-31","ZENO190008","Completed","2019-08-06","No","No","No","Internal"]
[null,null,null,null,2831,"36_14/10/2019 12:00:44 AM","2019-04-30","Defect","Ship Staff","Ship Staff Insp.","Atmospheric condenser inlet end cover found wasted","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","External Factors","8.16","Very High","","","same been renewed with fabricated one","2019-09-15","","Completed","2019-09-15","No","No","No","Internal"]
[null,null,null,null,2784,"36_14/10/2019 12:15:59 AM","2019-04-30","Defect","Ship Staff","Ship Staff Insp.","AE #2 LO inlet temperature sensor malfunctioning ","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","8.13","Medium","","","Sensor renewed.","2019-10-15","ZENO190007","Completed","2019-10-07","No","No","No","Internal","Pending items 2,3,6 & 7 delivered o/b at Singapore on 30062019. Pls revert with status of sensor renewal.\n"]
[null,null,null,null,2802,"36_13/10/2019 4:47:13 PM","2019-04-30","Defect","Ship Staff","Ship Staff Insp.","AE # 1 jacket cooling water outlet temp gauge found malfunctioning","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.21","Medium","","","same been renewed with new one","2019-05-31","ZENO1950101","Completed","2019-05-25","No","No","No","Internal"]
[null,null,null,null,2803,"36_13/10/2019 4:50:32 PM","2019-04-30","Defect","Ship Staff","Ship Staff Insp.","AE # 2 jacket cooling water outlet gauge malfunctioning","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.21","Medium","","","same been renewed with spare recieved","2019-05-31","ZENO195010","Completed","2019-05-25","No","No","No","Internal"]
[null,null,null,null,2804,"36_13/10/2019 4:54:15 PM","2019-04-30","Defect","Ship Staff","Ship Staff Insp.","AE # 3 jacket cooling water outlet gauge malfunctioning","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.21","Medium","","","same been renewed with spare recieved","2019-05-31","ZENO195010","Completed","2019-05-25","No","No","No","Internal"]
[null,null,null,null,8969,"36_Thu Dec 05 2019 16:24:17 GMT+0000 (Coordinated Universal Time)","2019-05-04","Non Conformity","Ship Staff","Nav Audit / Verification","No record of cancelled Navtex messages","Documentation","Navigation","Inappropriate Procedure","4.13","Very High","","","All cancelled Navtex messages to be deleted from ECDIS.                                                                          All navigating officers informed to maintain a NAVTEX file as per NAV AREAS and start maintaining records so that we do not miss out any cancelled Navtex mesages hence forth.","2019-05-10","","Completed","2019-05-08","No","No","No","Internal"]
[null,null,null,null,8188,"36_Thu Dec 05 2019 16:08:34 GMT+0000 (Coordinated Universal Time)","2019-05-04","Defect","Ship Staff","Nav Audit / Verification","Compass error not taken after large alteration of course","Documentation","Navigation","Behaviour Based,Human Error","4.9","Medium","","","OOW made aware to take compass error when ever there is alteration of more than 50 degrees is done.                                                                 Second officer advised to do a marking on ECDIS stating Compass error to be taken whenever there is alteration of more than 50 degrees.","2019-05-10","","Completed","2019-05-08","No","No","No","Internal"]
[null,null,null,null,8189,"36_Sun May 12 2019 16:12:21 GMT+0000 (Coordinated Universal Time)","2019-05-04","Defect","Ship Staff","Nav Audit / Verification","Off course alarm not tested on daily basis","Navigation - Others","Navigation","Inappropriate Procedure","4.7","High","","","All navigating officers told that off course alarm has to be tested daily and not on weekly basis.              Off course alarm check to be done at noon on daily basis.\n\nAll navigating officers told to hand over the same to the incoming officers so that this is not missed by the new officers on board.","2019-05-10","","Completed","2019-05-08","No","No","No","Internal"]
[null,null,null,null,8190,"36_Sun May 12 2019 16:24:17 GMT+0000 (Coordinated Universal Time)","2019-05-04","Non Conformity","Ship Staff","Nav Audit / Verification","No record of cancelled Navtex messages","Documentation","Navigation","Inappropriate Procedure","4.12","Very High","","","All cancelled Navtex messages to be deleted from ECDIS.                                                                          All navigating officers informed to maintain a NAVTEX file as per NAV AREAS and start maintaining records so that we do not miss out any cancelled Navtex mesages hence forth.","2019-05-10","","Completed","2019-05-08","No","No","No","Internal"]
[null,null,null,null,2817,"36_13/10/2019 7:10:35 PM","2019-05-15","Defect","Ship Staff","Ship Staff Insp.","Fire station general alarm push button missing from takeover","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.35","Medium","","","same been renewed with new one recieved","2019-07-31","ZENO190166","Completed","2019-07-20","No","No","No","Internal"]
[null,null,null,null,2823,"36_13/10/2019 9:50:54 PM","2019-05-15","Defect","Ship Staff","Ship Staff Insp.","AE local panel audible and visual alarm malfunctioning ","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.21","Medium","","","local panel vell and light been renewed with spare","2019-07-31","ZENO195045","Completed","2019-07-28","No","No","No","Internal"]
[null,null,null,null,2824,"36_13/10/2019 10:00:58 PM","2019-05-15","Defect","Ship Staff","Ship Staff Insp.","AE#3 LO cooler gasket leaking ","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","same been renewed with new one recieved","2019-07-31","ZENO190162","Completed","2019-08-02","No","No","No","Internal"]
[null,null,null,null,2827,"36_13/10/2019 11:26:47 PM","2019-05-15","Defect","Ship Staff","Ship Staff Insp.","AE#2 LO cooler gasket oil side leaking","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","same gasket been renewed","2019-07-31","ZENO190162","Completed","2019-08-07","No","No","No","Internal"]
[null,null,null,null,2832,"36_14/10/2019 12:04:33 AM","2019-05-15","Defect","Ship Staff","Ship Staff Insp.","Atmospheric condenser sw outlet valve found not holding same need to be renewed ","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","8.16","Very High","","","same been renewed","2019-09-15","","Completed","2019-08-27","No","No","No","Internal"]
[null,null,null,null,2808,"36_13/10/2019 6:10:02 PM","2019-05-15","Defect","Ship Staff","Ship Staff Insp.","PA speaker in monkey island not functioning","Elect. Mach. & Equip.","Communication","Equipment Related","","","","","same been rectified","2019-06-30","","Completed","2019-06-26","No","No","No","Internal"]
[null,null,null,null,2809,"36_13/10/2019 6:18:02 PM","2019-05-15","Defect","Ship Staff","Ship Staff Insp.","Deck foam pump recirculation line drain valve found leaking ","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.35","Medium","","","same been renewed with new one","2019-06-30","","Completed","2019-05-15","No","No","No","Internal"]
[null,null,null,null,2812,"36_13/10/2019 6:48:36 PM","2019-05-15","Breakdown","Ship Staff","Ship Staff Insp.","Sewage treatment plant air blower no# 1 impeller and casing found in seized condition","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","same been renewed with new one recieved ","2019-07-31","ZENO190168","Completed","2019-07-12","No","No","No","Internal"]
[null,null,null,null,2814,"36_13/10/2019 6:57:13 PM","2019-05-15","Defect","Ship Staff","Ship Staff Insp.","WBT tachometer PCB malfunctioning","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.8","Medium","","","same been recieved with spare recieved","2019-07-31","ZENO190175","Completed","2019-07-14","No","No","No","Internal"]
[null,null,null,null,2815,"36_13/10/2019 7:01:02 PM","2019-05-15","Defect","Ship Staff","Ship Staff Insp.","PP room fixed gas system relay for audible and visual alarm faulty","Elect. Mach. & Equip.","Cargo / Ballast Systems","Equipment Related","8.46","Very High","","","relay been renewed with spare recieved ","2019-07-31","ZENO190118/195053","Completed","2019-07-15","No","No","No","Internal"]
[null,null,null,null,2819,"36_13/10/2019 7:26:34 PM","2019-05-17","Defect","Ship Staff","Ship Staff Insp.","Elevator inverter malfunctioning(sliding door PCB malfunctioning)","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","PCB unit card renewed ","2019-07-31","ZENO190181","Completed","2019-07-24","No","No","No","Internal"]
[null,null,null,null,2828,"36_13/10/2019 11:50:42 PM","2019-05-17","Defect","Ship Staff","Ship Staff Insp.","IG scrubber tower nozzle cooling section pipe got corroded","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.31","Very High","","","corroded nozzle  cooling pipe renewed","2019-07-31","","Completed","2019-08-15","No","No","No","Internal"]
[null,null,null,null,2820,"36_13/10/2019 8:41:44 PM","2019-05-31","Defect","Ship Staff","Ship Staff Insp.","Aux.blr UNI SAAB Controller battery expired","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","Battery renewed 3Pc","2019-07-31","ZENO190180","Completed","2019-07-24","No","No","No","Internal"]
[null,null,null,null,2830,"36_13/10/2019 11:57:34 PM","2019-05-31","Defect","Ship Staff","Ship Staff Insp.","Steering gear #1 tank gauge glass and level alarm indicator oil leakage ","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","oil tank emptied and o ring renewed","2019-08-31","","Completed","2019-08-20","No","No","No","Internal"]
[null,null,null,null,2810,"36_13/10/2019 6:28:37 PM","2019-05-31","Breakdown","Ship Staff","Ship Staff Insp.","AE # 1 crankshaft and journal wear down excessively need to renew","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","same been renewed with spare recieved ","2019-06-30","ZENO195057","Completed","2019-07-11","No","No","No","Internal"]
[null,null,null,null,2807,"36_13/10/2019 6:06:21 PM","2019-06-10","Defect","Ship Staff","Ship Staff Insp.","2P bunker tank vent head found badly corroded from joints","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","Equipment Related","11.7","High","","","same been taken to E/R workshop,welding carried out and fitted back","2019-06-15","","Completed","2019-06-26","No","No","No","Internal"]
[null,null,null,null,2816,"36_13/10/2019 7:06:21 PM","2019-06-25","Defect","Ship Staff","Ship Staff Insp.","COPT air ejector steam inlet vv found leaking from the gasket","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","same gasket been renewed","2019-07-31","","Completed","2019-07-17","No","No","No","Internal"]
[null,null,null,null,2829,"36_13/10/2019 11:54:00 PM","2019-06-26","Defect","Ship Staff","Ship Staff Insp.","FWG ejector pump discharge valve not holding ","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.31","Very High","","","same been renewed with new one","2019-08-31","","Completed","2019-08-19","No","No","No","Internal"]
[null,null,null,null,2821,"36_13/10/2019 8:52:14 PM","2019-07-08","Defect","Ship Staff","Ship Staff Insp.","Rescue boat canopy light not working","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.28","Very High","","","same been renewed with new one","2019-07-31","ZENO190236","Completed","2019-07-25","No","No","No","Internal"]
[null,null,null,null,14243,"36_1 Oct 2020 1:06:35 PM","2019-07-09","Breakdown","Ship Staff","Ship Staff Insp.","Lifeboat Line Floaters, Inboard side were found damaged, to be renewed","LSA / FFA","Safety / LSA / FFA","External Factors","5.29","High","","","Inboard side renewed, ouboard side inspected, found in good condition","2020-10-31","","Completed","2020-09-30","No","No","No","Internal"]
[null,null,null,null,8181,"36_Sun May 12 2019 04:20:36 GMT+0000 (Coordinated Universal Time)","2019-07-09","Defect","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","High expansion foam tank in the steering gear room was not clearly marked with works on piping and observed wrong marking and not distigushed colour code from the fire line","LSA / FFA","General Appearance","Behaviour Based","5.38","High","","","Remarked the foam line in distiguished color arrow marks. Inspected the other markings on fire and foam line , Same was found in order","2019-07-20","","Completed","2019-07-12","No","No","No","External"]
[null,null,null,null,8182,"36_Sun May 12 2019 04:29:34 GMT+0000 (Coordinated Universal Time)","2019-07-09","Defect","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","Lamp holding bracket was almost brocken condition for an emergency light fitted on upper deck starboard side , out side accommodation","Elect. Mach. & Equip.","Structural Condn. / WT integrity ","Equipment Related","11.9","Low","","","After deparure from the Discharge port old bracket and emergency light removed and replaced with the new bracket and emergency light.All the remaining light fixtures were inspected and found in satisfactory condition.","2019-07-12","","Completed","2019-07-12","No","No","No","External"]
[null,null,null,null,8183,"36_Thu Dec 05 2019 05:44:41 GMT+0000 (Coordinated Universal Time)","2019-07-09","Defect","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)"," Pumping Log was not maintained even 5 hours passed since cargo\n\ncommenced and there was no record evidence of cargo pumps started even on the cargo\n\noperation record book while discharging operation.","Miscellaneous","ISM Related","Human Error,Inappropriate Procedure","8.7","High","","","Pumping log was completed immediately .Training given to all duty officers regarding the entries to be made in the cargo log books.","2019-07-09","","Completed","2019-07-09","No","No","No","External"]
[null,null,null,null,8192,"36_Sun May 12 2019 16:44:08 GMT+0000 (Coordinated Universal Time)","2019-07-24","Non Conformity","Ship Staff","Nav Audit / Verification","Reference to Navigation Audit Checklist 58: No entry related to Auto Pilot operation tested on TMC could be found.  ","Navigation - Others","Navigation","Human Error,Inappropriate Procedure","4.1","High","","","Immediately Entry made in Deck Log book. Varified that during weekly routine the same entry to be made in Deck log book.","2019-10-24","","Completed","2019-08-20","No","No","No","Internal"]
[null,null,null,null,8963,"36_Sun May 12 2019 15:15:21 GMT+0000 (Coordinated Universal Time)","2019-07-24","Defect","Owner / Marine / Tech. Suptd.","ISM Audit","Funnel deck, 15 number of Lube Oil drums stowed on open deck with inadequate lashing arrangement.","Miscellaneous","ISM Related","Behaviour Based,Inappropriate Procedure","5.11","Low","","","All the drums were properly lashed with wire lashing and covered with canvas so that it looks tidy.","2019-10-24","","Completed","2019-07-31","No","No","No","Internal"]
[null,null,null,null,8196,"36_Sun May 12 2019 16:30:51 GMT+0000 (Coordinated Universal Time)","2019-07-24","Defect","Ship Staff","Nav Audit / Verification","Reference to Navigation Audit Checklist column 11: Navigation equipment maintenance entry could not be found in Deck Log Book.","Documentation","Navigation","Inappropriate Procedure","4.1","High","","","immediately entry made of the maintenance carried out in Deck log book,                                      During Daily and Weekly Maintenance routine  entry of the same to be carried out in Deck log boo","2019-10-24","","Completed","2019-08-20","No","No","No","Internal"]
[null,null,null,null,8964,"36_Thu Dec 05 2019 15:21:49 GMT+0000 (Coordinated Universal Time)","2019-07-24","Non Conformity","Owner / Marine / Tech. Suptd.","ISM Audit","Working life vest was not provided to shore people coming on board. ","Miscellaneous","ISM Related","Inappropriate Procedure","5.47","Medium","","","Crew and officers were advised to ensure that working lifevest is given to all personnel prior boarding the vessel. Same was cross checked and ensured at Bonny terminal, that vessel provided working lifevests to shore personnel prior boarding.   Crew and officers were explained about the importance and significance of a lifevest during the boarding.","2019-10-24","","Completed","2019-09-09","No","No","No","Internal"]
[null,null,null,null,8965,"36_Thu Dec 05 2019 15:32:07 GMT+0000 (Coordinated Universal Time)","2019-07-24","Defect","Owner / Marine / Tech. Suptd.","ISM Audit","U-Clamps in front of pump room, on steam line, found to be corroded. Need to de-rust and paint. ","Deck - Pipe / Fittings","General Appearance","Inappropriate Procedure","8.17","Low","","","The job of de-rusting the U-Clamps was taken up as soon as the vessel departed.                                  A thorough inspection was carried out for all clamps and lines, rusted clamps were identified and the de-rusting of same was done in a systematic manner.  ","2019-10-24","","Completed","2019-08-08","No","No","No","Internal"]
[null,null,null,null,8966,"36_Thu Dec 05 2019 15:37:39 GMT+0000 (Coordinated Universal Time)","2019-07-24","Non Conformity","Owner / Marine / Tech. Suptd.","Nav Audit / Verification","ENC Chart on arrival route, near Horsburgh Light House was not identified in passage plan as chart was of different datum than WGS-84.","Documentation","Navigation","Human Error,Inappropriate Procedure","4.16","Very High","","","Entire route was checked immediately and all the charts were identified, They were marked using user chart, precautionary note was written: positions to be verified by fix objects using visual bearing and radar ranges.","2019-10-24","","Completed","2019-07-24","No","No","No","Internal"]
[null,null,null,null,8967,"36_Thu Dec 05 2019 15:45:47 GMT+0000 (Coordinated Universal Time)","2019-07-24","Non Conformity","Owner / Marine / Tech. Suptd.","Nav Audit / Verification","Astern Light angle found to be more than 135deg. Urgently need to be attended upon departure.","Navigation - Others","Navigation","Equipment Related","4.8","Medium","","","Astern light lantern was removed from location. Angles measured, checked and found all in order. ","2019-10-24","","Completed","2019-10-26","No","No","No","Internal"]
[null,null,null,null,8176,"36_Sun May 12 2019 15:37:39 GMT+0000 (Coordinated Universal Time)","2019-07-24","Non Conformity","Owner / Marine / Tech. Suptd.","Nav Audit / Verification","ENC Chart on arrival route, near Horsburgh Light House was not identified in passage plan as chart was of different datum than WGS-84.","Documentation","Navigation","Human Error,Inappropriate Procedure","","","","","Entire route was checked immediately and all the charts were identified, They were marked using user chart, precautionary note was written: positions to be verified by fix objects using visual bearing and radar ranges.","2019-10-24","","Completed","2019-07-24","No","No","No","Internal"]
[null,null,null,null,8184,"36_Thu Dec 05 2019 15:15:21 GMT+0000 (Coordinated Universal Time)","2019-07-24","Defect","Owner / Marine / Tech. Suptd.","ISM Audit","Funnel deck, 15 number of Lube Oil drums stowed on open deck with inadequate lashing arrangement.","Miscellaneous","ISM Related","Behaviour Based,Inappropriate Procedure","","","","","All the drums were properly lashed with wire lashing and covered with canvas so that it looks tidy.","2019-10-24","","Completed","2019-07-31","No","No","No","Internal"]
[null,null,null,null,8185,"36_Sun May 12 2019 15:21:49 GMT+0000 (Coordinated Universal Time)","2019-07-24","Non Conformity","Owner / Marine / Tech. Suptd.","ISM Audit","Working life vest was not provided to shore people coming on board. ","Miscellaneous","ISM Related","Inappropriate Procedure","","","","","Crew and officers were advised to ensure that working lifevest is given to all personnel prior boarding the vessel. Same was cross checked and ensured at Bonny terminal, that vessel provided working lifevests to shore personnel prior boarding.   Crew and officers were explained about the importance and significance of a lifevest during the boarding.","2019-10-24","","Completed","2019-09-09","No","No","No","Internal"]
[null,null,null,null,8186,"36_Sun May 12 2019 15:32:07 GMT+0000 (Coordinated Universal Time)","2019-07-24","Defect","Owner / Marine / Tech. Suptd.","ISM Audit","U-Clamps in front of pump room, on steam line, found to be corroded. Need to de-rust and paint. ","Deck - Pipe / Fittings","General Appearance","Inappropriate Procedure","","","","","The job of de-rusting the U-Clamps was taken up as soon as the vessel departed.                                  A thorough inspection was carried out for all clamps and lines, rusted clamps were identified and the de-rusting of same was done in a systematic manner.  ","2019-10-24","","Completed","2019-08-08","No","No","No","Internal"]
[null,null,null,null,8187,"36_Sun May 12 2019 15:45:47 GMT+0000 (Coordinated Universal Time)","2019-07-24","Non Conformity","Owner / Marine / Tech. Suptd.","Nav Audit / Verification","Astern Light angle found to be more than 135deg. Urgently need to be attended upon departure.","Navigation - Others","Navigation","Equipment Related","","","","","Astern light lantern was removed from location. Angles measured, checked and found all in order. ","2019-10-24","","Completed","2019-10-26","No","No","No","Internal"]
[null,null,null,null,8191,"36_Sun May 12 2019 16:35:49 GMT+0000 (Coordinated Universal Time)","2019-07-24","Non Conformity","Ship Staff","Nav Audit / Verification","Reference to Navigation Audit Checklist 12.2: Entry related to verifying of Ship heading with Navigation  equipment like Ecdis, Radar, Ais could be sighted. No records found.","Documentation","Navigation","Inappropriate Procedure","4.1","High","","","Immediately made entry in Log book . Started to make daily entries in log book","2019-10-24","","Completed","2019-08-20","No","No","No","Internal"]
[null,null,null,null,2791,"36_14/10/2019 8:42:35 AM","2019-08-02","Defect","Ship Staff","Ship Staff Insp.","MIC for talk balk system in the steering gear found not working","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","4.7","High","","","same need to be renewed","2019-10-15","ZENO190246","Completed","2019-10-26","No","No","No","Internal"]
[null,null,null,null,11394,"36_14 Feb 2020 10:30:45 AM","2019-08-23","Breakdown","Ship Staff","Ship Staff Insp.","Accommodation Fixed Gas Detection System inoperational. System need to be Upgraded.","Accommodation","Safety / LSA / FFA","Equipment Related","5.22","High","","","Spares recieved, job is in progress.","2021-01-10","","Completed","2021-01-05","No","No","No","Internal","Rajiv, Master advises that no technician had attended on board for same. Pls advice."]
[null,null,null,null,17359,"36_15/1/2021 6:01:09 PM","2019-08-26","Observation","Ship Staff","Ship Staff Insp.","STARBOARD SIDE PILOT LADDER OF NON-COMPLIANT TYPE","Documentation","Cert. & Docu.","Equipment Related","","","","","Discussed with ops, Ladder is compliant and certified therefore can be used.","2020-10-10","","Completed","2020-09-15","No","No","No","Internal"]
[null,null,null,null,8195,"36_Wed Jun 12 2019 15:55:38 GMT+0000 (Coordinated Universal Time)","2019-09-02","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Remote Audit- \n\nArrival  condition to be entered in CCR Record book along with EOSP . 12.21.06.001.01 - Guidelines for making entries in logbook to be followed.","Documentation","Cargo / Ballast Systems","Behaviour Based,Human Error","8.5","Very High","","","CCR Log book entered with the arrival condition on later page.Training given to concerned persons on the entries to be made in the CCR log book. Entries verified in the next arrival and found in compliance.","2019-09-13","","Completed","2019-09-13","No","No","No","Internal"]
[null,null,null,null,2792,"36_14/10/2019 8:44:59 AM","2019-09-12","Defect","Ship Staff","Ship Staff Insp.","Main engine turning gear remote cable male plug found damaged","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Renewed.","2019-12-15","ZENO190268","Completed","2020-01-19","No","No","No","Internal",""]
[null,null,null,null,11395,"36_14 Feb 2020 10:24:18 AM","2019-10-09","Breakdown","Ship Staff","Ship Staff Insp.","H2S Sensor (reading) for pumproom fixed Gas detection system not working. The system is obselete and will need renewal as per Service report.","Cargo Mach.","Safety / LSA / FFA","Equipment Related","5.21","Medium","","","Awaiting Renewal/repair for the system.On 09th May-2020 System was completely renewed .Working Satisfactory.","2020-05-30","ZENO205031/","Completed","2020-05-09","No","No","No","Internal"]
[null,null,null,null,8194,"36_Fri Dec 06 2019 03:14:45 GMT+0000 (Coordinated Universal Time)","2019-11-12","Defect","Ship Staff","Mooring Audit","Equipment No in ships MSMP mentioned as 5253.3 As per IMO circular calculated EQ no is 5253.3 where as , as per design anchor handling plan equipment no is provided as 5231.68","Documentation","Mooring","Human Error,Inappropriate Procedure","9.2","Very High","","","Equipment number changed in the MSMP .Minimum breaking strength of mooring ropes updated as per EN.Inspected the MSMP for further errors. updated as required. ","2019-11-20","","Completed","2019-11-14","No","No","No","Internal"]
[null,null,null,null,8197,"36_Wed Jun 12 2019 16:14:33 GMT+0000 (Coordinated Universal Time)","2019-11-12","Defect","Ship Staff","Mooring Audit","Anchor windlass break lining found thinned out . Require renewal","Deck - Mooring Machinery","Mooring","Equipment Related","9.15","Medium","","","Port anchor was secured using extra lashing, requisition raised for brake linning for both the anchors. Expected to receive in Rotterdam on 16 Dec 2019.","2020-01-12","","Completed","2019-12-06","No","No","No","Internal"]
[null,null,null,null,8177,"36_Wed Jun 12 2019 16:11:35 GMT+0000 (Coordinated Universal Time)","2019-11-12","Defect","Ship Staff","Mooring Audit","As a good practice mooring tail eye should be covered with canvas or rubber kind of material to prevent chaffing on the terminal bits. Mooring tails found not covered appropriately.","Deck - Mooring Machinery","Mooring","Inappropriate Procedure","9.5","High","","","Canvas stitched for all the mooring tails.","2020-01-12","","Completed","2019-12-21","No","No","No","Internal","Please complete this job at the earliest."]
[null,null,null,null,10362,"36_25 Jan 2020 11:16:57 AM","2019-11-14","Breakdown","Ship Staff","Engineering Audit","Incinerator not operational due to defective burner control.","E/R - Aux. Mach.,Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Spares being awaited.","2019-12-20","ZENO190292","Completed","2020-01-16","No","No","No","Internal"]
[null,null,null,null,10363,"36_25 Jan 2020 11:45:07 AM","2019-11-25","Breakdown","Ship Staff","Ship Staff Insp.","AE2 LO Cooler leaking due to damaged plates.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Deformed plates straightened. Changed the gaskets with new set of gaskets. Plates slips out of the stack. Put back the old gaskets. Plates to be renewed.","2019-12-20","ZENO190296","Completed","2020-01-16","No","No","No","Internal"]
[null,null,null,null,10364,"36_25 Jan 2020 11:49:53 AM","2019-11-30","Breakdown","Ship Staff","Ship Staff Insp.","Aux engine 3 Unit 4 High exhaust gas temperature due to burned exhaust valve.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Cylinder head to replace with an Overhauled spare. Cylinder head replaced with an overhauled spare.","2019-12-02","","Completed","2019-12-02","No","No","No","Internal"]
[null,null,null,null,10365,"36_25 Jan 2020 11:54:22 AM","2019-12-02","Breakdown","Ship Staff","Engineering Audit","Sewage treatment plant no.1 air blower motor is defective.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Motor to be renewed.","2020-01-16","ZENO190301","Completed","2020-01-24","No","No","No","Internal"]
[null,null,null,null,10366,"36_25 Jan 2020 11:58:11 AM","2019-12-08","Defect","Ship Staff","Engineering Audit","Sacrificial flanges on both LT Coolers sea water inlet pipe found leaking.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Flanges to renew. Flanges renewed. Rectified the leak.","2019-12-15","","Completed","2019-12-12","No","No","No","Internal"]
[null,null,null,null,10367,"36_25 Jan 2020 12:01:35 PM","2019-12-16","Observation","Ship Staff","Ship Staff Insp.","Fwd hydraulic cooling water line leaking.","Deck - Mooring Machinery","Mooring","Equipment Related","9.14","Medium","","","Pipeline section dismanteled, leak arrested and fixed back. Tested with sea water running, no leak found.","2020-03-16","","Completed","2019-12-26","No","No","No","Internal"]
[null,null,null,null,10368,"36_25 Jan 2020 12:05:40 PM","2019-12-17","Breakdown","Ship Staff","Engineering Audit","No. 2 Vacuum pump motor for sewage collecting tank found trippeddue to overload.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Motor to overhaul. Pump was tripping due to deposit formation in the bearing bush. Same polished. Motor overhauled by renewing the ball bearings as same found running noisy.","2019-12-20","","Completed","2019-12-18","No","No","No","Internal"]
[null,null,null,null,11392,"36_12 Feb 2020 3:32:35 AM","2020-01-01","Breakdown","Ship Staff","Engineering Audit","No 2 Oxygen analyser is defective.","Cargo Mach.,Inert Gas","Eng. / Strg. Comp.","Equipment Related","8.26","High","","","Spare unit recieved and installed, job completed.now both units are functional.","2020-12-30","ZENO190223.","Completed","2020-12-30","No","No","No","Internal","Will check repair status of same & revert."]
[null,null,null,null,10361,"36_25 Jan 2020 12:11:22 PM","2020-01-13","Defect","Ship Staff","Mooring Audit","Anchor windlass port side brake lining thinned down, need renewal.","Deck - Mooring Machinery","Mooring","Equipment Related","9.15","Medium","","","Port anchor secured using extra lashing. Brake lining received at rotterdam. Renewed brake lining on 12 Feb 2020. Brakes tried out on 14 Feb 2020, found satisfactory.","2020-02-12","ZENO190309","Completed","2020-02-12","No","No","No","Internal"]
[null,null,null,null,11396,"36_12/02/2020 15:16:12","2020-01-16","Defect","Ship Staff","Ship Staff Insp.","AUS Solenoid valve leaking air.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.8","Medium","","","AUS Solenoid valve to be renewed.Spare received fitted in place.Leak rectified.","2020-06-30","ZENO200010","Completed","2020-06-20","No","No","No","Internal","RO cancelled by Owner. Pls update on current status of the valve."]
[null,null,null,null,11405,"36_12/02/2020 15:03:57","2020-01-16","Defect","Ship Staff","Ship Staff Insp.","Stbd side pilot ladder in deteriorated condition, need renewal.","Navigation - Others","Safety / LSA / FFA","Equipment Related","5.47","Medium","",""," Pilot ladder replaced with new one ,received at Suez.","2020-05-01","ZENO200002","Completed","2020-03-11","No","No","No","Internal"]
[null,null,null,null,10369,"36_25 Jan 2020 12:15:49 PM","2020-01-18","Observation","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","Last annual calibration for alcohol meter was on 08 November 2018. The requisition for new sensor was sighted.","Miscellaneous","Cert. & Docu.","Equipment Related","3.8","Very High","","","New alcohol meter received on board with certificate.","2020-02-02","","Completed","2020-01-19","No","No","No","External"]
[null,null,null,null,10370,"36_25 Jan 2020 12:27:02 PM","2020-01-18","Observation","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","3 x Immersion suit in forecastle space and 2 x EEBD in Cargo pump room were not marked with IMO Symbol on the doors to the entrance indicating the devices stored in the location. Rectified immediately when pointed out.","LSA / FFA","Safety / LSA / FFA","External Factors,Human Error","5.31","High","","","Immediately IMO Symbols pasted in position at entrance of pump room and Forecastle store.","2020-02-02","","Completed","2020-01-18","No","No","No","External"]
[null,null,null,null,11401,"36_14 Feb 2020 2:26:16 AM","2020-02-01","Defect","Ship Staff","Engineering Audit","AE3 lub oil cooler plates are damaged causing LO leak from LO cooler during engine operation.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Saveall fabricated below the cooler to contain the leak. Requisition raised for a complete set of plates. Spares received on 09th May-2020.Fitted in place D/G tried out running satisfactory.","2020-05-15","ZENO200020","Completed","2020-05-14","No","No","No","Internal"]
[null,null,null,null,11403,"36_12 Feb 2020 3:16:19 AM","2020-02-08","Defect","Ship Staff","Engineering Audit","Main engine Viscometer not working","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Viscometer to check/ overhaul.Overhauled ,giving correct readings but still under observation.Working Satisfactory.","2020-05-31","","Completed","2020-05-20","No","No","No","Internal","Please advice outcome of the observation. If unit working normally, please close out defect."]
[null,null,null,null,11402,"36_12/02/2020 15:53:29","2020-02-10","Breakdown","Ship Staff","Ship Staff Insp.","MF/ HF Transmission failure . Vessel is not receiving MF/HF shore acknowledgment. ","Navigation - GMDSS & Communication","Navigation","Equipment Related","4.23","High","","","Close inspection carried out on the system , ATU PCB found burned. Damege reported to office.Awaiting technision.Technician attended the vessel.Job completed at Singapore.","2020-05-10","ZENO205022- Technician attended the vessel.","Completed","2020-04-03","No","No","No","Internal"]
[null,null,null,null,11404,"36_12 Feb 2020 3:20:52 AM","2020-02-11","Other","Ship Staff","Engineering Audit","ME Unit 4 and 6 Fuel pump shock absorber causing jerk on the fuel inlet pipe to the high pressure pump.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Overhaul the fuel pump shock absorbers.","2020-03-10","","Completed","2020-02-14","No","No","No","Internal"]
[null,null,null,null,11398,"36_26 Feb 2020 10:17:53 PM","2020-02-16","Defect","Ship Staff","Engineering Audit","AC compressor 2 showing high suction pressure. Compressor running with less cooling effect. Suspect Unloader or valve plate brekage. ","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Compressor to dismantle ans inspect/ repair.Compressor suction discharge valves overhauled.Referigerant charged .Oil renewed.Compressor running satisfactorily.","2020-06-15","","Completed","2020-06-04","No","No","No","Internal","Please revert with inspection / repair status of the unit.\nWhen do you plan to inspect / repair the unit.  Presume all spares are already available on board since no PO issued for same."]
[null,null,null,null,11399,"36_26 Feb 2020 10:11:12 PM","2020-02-26","Critical Equipment","Ship Staff","Engineering Audit","OWS data recorder oil content PPM reading is erratic.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","6.14","High","","","New ABS data recorder received and fitted.Oil content  is showing correct.","2020-04-15","ZENO200039","Completed","2020-04-03","No","No","No","Internal"]
[null,null,null,null,12208,"36_15/5/2020 7:25:50 PM","2020-04-04","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Fresh water generator production is low and needs to be improved","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.1","Medium","","","FWG condenser evaporator cleaned. Monitored the performance.Working Satisfactory.","2020-06-15","","Completed","2020-06-02","No","No","No","Internal","This defect was recorded in April 2020 but to date still not started. Pls advice reason for delay in carrying out the required action."]
[null,null,null,null,12209,"36_15/5/2020 7:00:50 PM","2020-04-04","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Emergency Fire pump vacuum pump(Q-vac) to be overhauled","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","5.41","Very High","","","Q-Vac pump overhauled. ","2020-06-15","","Completed","2020-06-09","No","No","No","Internal","Please advice reason for delay in overhauling the pump. Since there is no  P.O. ref no. indicated, prsume you are not waiti pang for spares delivery."]
[null,null,null,null,12210,"36_15/5/2020 7:33:33 PM","2020-04-04","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","M/E foundation bolts rusted.To be cleaned and greased","E/R - Main Engine","General Appearance","Equipment Related","10.1","Medium","","","Foundation bolts of M/E Cleaned and greased.","2020-05-31","","Completed","2020-05-25","No","No","No","Internal","Presume this job should have been completed by now. If not please justify delay in completion.  If already completed, we request that you close out this defect."]
[null,null,null,null,12214,"36_15/5/2020 6:47:50 PM","2020-04-04","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","COPT platform pressure gauges and electrical panels were found dirty.To be cleaned.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Cleaning completed on 01 May-2020","2020-04-30","","Completed","2020-05-02","No","No","No","Internal"]
[null,null,null,null,12215,"36_15/5/2020 7:14:16 PM","2020-04-04","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Engine room Bilges Port Side FWD filter casing and pipes and flanges to be de-rusted and painted","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Area de-rusted and painted.","2020-05-15","","Completed","2020-05-02","No","No","No","Internal"]
[null,null,null,null,12216,"36_15/5/2020 7:38:27 PM","2020-04-04","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","M/E F.O. supply pump seal lube oil pot to be filled up with oil.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.1","Medium","","","Seal lube oil Pot filled up with lube oil","2020-05-20","","Completed","2020-05-01","No","No","No","Internal"]
[null,null,null,null,17353,"36_15/1/2021 5:06:57 PM","2020-04-04","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","IG Branch Valves are leaking for all COT’s except for 5 Wings. This item is pending approval from Owners.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.33","Medium","","","New Valves recd and fitted.","2020-07-04","","Completed","2020-06-30","No","No","No","Internal"]
[null,null,null,null,17360,"36_15/1/2021 4:39:29 PM","2020-04-04","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Cable ducts and Conduit pipes are rusted. To be de rusted and painted ","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.4","Very High","","","Derusting and painting completed","2020-07-03","","Completed","2020-07-01","No","No","No","Internal"]
[null,null,null,null,17361,"36_15/1/2021 4:43:14 PM","2020-04-04","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Funnel stacks are dirty. To be cleaned and painted. Funnel bottom plating to be chipped and painted.  ","Miscellaneous","General Appearance","Equipment Related","11.8","Low","","","Spot chipping and painting carried out. ","2020-06-03","","Completed","2020-06-03","No","No","No","Internal"]
[null,null,null,null,17362,"36_15/1/2021 4:51:40 PM","2020-04-04","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Forecastle store to be cleaned and rearranged. ","Miscellaneous","General Appearance","Equipment Related","11.12","Low","","","Forecastle cleaned and arranged.","2020-05-20","","Completed","2020-05-13","No","No","No","Internal"]
[null,null,null,null,17363,"36_15/1/2021 5:00:53 PM","2020-04-04","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Pump room natural ventilation duct and flap rusted. To be de rusted and painted. ","Miscellaneous","General Appearance","Equipment Related","","","","","Derusting and painting carried out.","2020-06-03","","Completed","2020-06-03","No","No","No","Internal"]
[null,null,null,null,17364,"36_15/1/2021 5:03:37 PM","2020-04-04","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Gangway turn table underside is rusted. To be derusted and painted. ","Deck - Pipe / Fittings","General Appearance","Equipment Related","","","","","Deusting and painting carried out.","2020-06-03","","Completed","2020-06-03","No","No","No","Internal"]
[null,null,null,null,17365,"36_15/1/2021 5:10:10 PM","2020-04-04","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Cargo tank steam heating coils and valves need derusting and painting","Deck - Pipe / Fittings","General Appearance","Equipment Related","","","","","Derusting and painting carried out.","2020-07-03","","Completed","2020-07-03","No","No","No","Internal"]
[null,null,null,null,17366,"36_15/1/2021 5:17:08 PM","2020-04-04","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Paints found stored in the engine room. After completion of work these are to be transferred to the paint locker every day. ","Miscellaneous","Eng. / Strg. Comp.","Inappropriate Procedure","","","","","Paint drums cleared and transferred to the paint store.","2020-04-04","","Completed","2020-04-04","No","No","No","Internal"]
[null,null,null,null,17367,"36_15/1/2021 5:18:53 PM","2020-04-04","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ME Viscotherm found erratic. To be investigated","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Viscotherm cleaned . now working fine.","2020-05-20","","Completed","2020-04-15","No","No","No","Internal"]
[null,null,null,null,17368,"36_15/1/2021 5:37:55 PM","2020-04-04","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp."," No 2 O2 Analyser unit display unit keypad is not working. ","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","Unit replaced .","2020-06-03","","Completed","2020-05-15","No","No","No","Internal"]
[null,null,null,null,17369,"36_15/1/2021 4:57:44 PM","2020-04-04","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Spot rust visible forward of manifold area. To be de rusted and painted. ","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.3","Medium","","","Spot chipping and painting carried out.","2020-07-03","","Completed","2020-07-03","No","No","No","Internal"]
[null,null,null,null,17370,"36_15/1/2021 5:14:44 PM","2020-04-04","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ECR Control panels are dirty and require cleaning/","Elect. Mach. & Equip.","General Appearance","Equipment Related","","","","","Panels cleaned.","2020-05-20","","Completed","2020-05-15","No","No","No","Internal"]
[null,null,null,null,null,"36_22/3/2021 10:22:51 AM","2020-04-04","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","IG Branch Valves area leaking for all COT's Except for 5 Wings. This item is pending approval from owners.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related",8.33,"Medium","Not Applicable","Not Applicable","14 valves recvd, fitted on 1W, 2W, 3W, 4W, 5P, 6W & SLP-W. Remaining 1 valves Kept as spare as 5S IG valve codition noted to be good & holding.","2021-06-30",null,"Completed","2021-06-14","No",null,null,"Internal"]
[null,null,null,null,12211,"36_15/4/2020 4:56:31 PM","2020-04-08","Defect","Ship Staff","Ship Staff Insp.","E/R alarm monitoring system Resource station 2 Comm. Error. Secondary NET-MPM Defective.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.2","Low","","","Communication in progress with shore team/Spare received on 09th May-20.Fitted in place.All alarm got reset system is under observation.Working Satisfactory.","2020-06-30","ZENO205023","Completed","2020-06-18","No","No","No","Internal","Presume observation over a period of 01 month should be sufficient to verify if system is working fine. Please close-out defect if possible."]
[null,null,null,null,12213,"36_15/4/2020 6:05:05 PM","2020-04-13","Defect","Ship Staff","Ship Staff Insp.","S Band radar given RF error alarm and got powered of. Unable restart the Radar ","Navigation - RADAR","Navigation","Equipment Related","","","","","Service by shore technician arranged at Bayuquan port on 18 Apr 2020. Under observation.Now Working satisfactory.","2020-06-15","","Completed","2020-05-16","No","No","No","Internal","It is already more that 1.5 months since the attendance of a shore technician on board. Presume by now the observation period should be sufficient to verify if unit is functioning properly.  Pls close out defect if possible."]
[null,null,null,null,12212,"36_15/5/2020 8:06:33 PM","2020-05-09","Defect","Ship Staff","Ship Staff Insp.","Minor steam leak observed in purifier room at Ceiling.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Clamping arrangement made to arrest the leak.Gasket renewed.","2020-05-30","","Completed","2020-05-27","No","No","No","Internal","Please revert with progress status for same."]
[null,null,null,null,12217,"36_15/5/2020 7:51:23 PM","2020-05-09","Defect,Observation","Ship Staff","Ship Staff Insp.","Weather tight funnel door corroded at bottom need to be repair.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.44","Medium","","","To be repaired / To be Build up/On 11th May Door repaired in E/R workshop. ","2020-05-15","","Completed","2020-05-11","No","No","No","Internal"]
[null,null,null,null,13117,"36_8/6/2020 8:13:54 PM","2020-06-08","Observation","Ship Staff","Ship Staff Insp.","Aux. Boiler No.2 Heating steam inlet line valve leaking from galnd and Bonnet.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Leak rectified.","2020-06-18","","Completed","2020-06-17","No","No","No","Internal"]
[null,null,null,null,13338,"36_15/7/2020 3:46:24 PM","2020-07-15","Defect","Ship Staff","Ship Staff Insp.","Steam driven Water Ballast pump upper bearing temp. Switch/gauge is defective.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.13","Medium","","","Spares recieved and replaced. now all working good.","2021-01-15","ZENO200133","Completed","2021-01-05","No","No","No","Internal",""]
[null,null,null,null,13339,"36_30/7/2020 4:36:44 PM","2020-07-23","Defect","Ship Staff","Ship Staff Insp.","POWER SUPPLY UNIT OF E/R ALARM MONITORING SYSTEM IS DEFECTIVE.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.37","Medium","","","Spare recd and replaced, working satisfactory.","2020-08-20","ZENO200140","Completed","2020-08-30","No","No","No","Internal","Understand spares were supplied on board at Singapore on 26082020. Please provide update on rectification of the fault."]
[null,null,null,null,13340,"36_30/7/2020 4:47:09 PM","2020-07-27","Defect","Ship Staff","Ship Staff Insp.","Galley Oven heating coil is defective giving 440 V AC low insulation alarm.","Accommodation","Eng. / Strg. Comp.","Equipment Related","10.38","Medium","","","Spare coils recieved, job completed.","2021-01-25","ZENO200141","Completed","2021-06-06","No","No","No","Internal","Based on VFF, the order was supplied by Owner on 19th Dec 2020 @ Singapore. What action have been taken to date to rectify the defect?"]
[null,null,null,null,13343,"36_30/7/2020 4:54:37 PM","2020-07-27","Defect","Ship Staff","Ship Staff Insp.","Negative phase relay of FWD Electric Whistle is giving 440 V AC low insulation alarm while operating.","Deck - Machinery,Navigation - Others","Eng. / Strg. Comp.","Equipment Related","10.38","Medium","","","Sapres recd. Fwd whistle overhauled and all parts renewed as found damaged, whistle fixed and tried.","2020-09-30","ZENO200093","Completed","2020-09-15","No","No","No","Internal","Understand spares were supplied on board at Singapore on 26082020.\nPlease provide update on replacing of the phase relay."]
[null,null,null,null,13341,"36_4/8/2020 3:24:27 PM","2020-08-04","Defect","Ship Staff","Ship Staff Insp.","#2 Bilge Bilge fire and GS Pump MCCB is defective","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.37","Medium","","","MCCB has been replaced with Equivalent rating MCCB. pump working fine.","2021-01-15","ZENO200146","Completed","2021-01-05","No","No","No","Internal",""]
[null,null,null,null,13342,"36_4/8/2020 3:41:08 PM","2020-08-04","Observation","Ship Staff","Ship Staff Insp.","Air Line on Stbd. Bridge Wing is leaking minutely, Noticed valve is defective","Miscellaneous","General Appearance","Equipment Related","11.4","Very High","","","Valve Renewed, tested, no more leaks","2020-10-31","-----","Completed","2020-09-28","No","No","No","Internal","Please revert with updated status on progress of the repairs."]
[null,null,null,null,13344,"36_4/8/2020 3:01:56 PM","2020-08-04","Defect","Ship Staff","Ship Staff Insp.","Fwd. Electric horn is not working","Deck - Machinery","Navigation","Equipment Related","","","","","spares recd and horn overhauled, all parts renewed as found damaged.","2020-09-28","ZENO200125","Completed","2020-09-14","No","No","No","Internal","To be Arranged by Owners… DTS sent to NF.MAWB NO. 180 7103 5016\nPls advice if the spares were supplied on board @ S'pore on 26082020."]
[null,null,null,null,13345,"36_4/8/2020 3:15:22 PM","2020-08-04","Observation","Ship Staff","Ship Staff Insp.","BIlge Fire and GS Pump discharge manifold line holed.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.31","Very High","","","Job completed and system tested to maximum working pressure. Satisfactory.","2020-11-30","","Completed","2020-11-01","No","No","No","Internal","Please revert with update."]
[null,null,null,null,14244,"36_30 Sep 2020 8:30:52 AM","2020-08-05","Defect","Ship Staff","Ship Staff Insp.","Securing Eye for Port Provision Crane observed broken, Crane Hook is secured on Railing, with rope","Deck - Machinery","Structural Condn. / WT integrity ","Equipment Related","","","","","Hot Work Permission obtained from Company & New Eye Welded, on 28 Sep 2020. Job Complete","2020-09-30","","Completed","2020-09-28","No","No","No","Internal"]
[null,null,null,null,13736,"36_2 Sep 2020 10:41:30 AM","2020-08-05","Defect","Ship Staff","Ship Staff Insp.","Deck Air Compressor : Non-operational for a long time, Deck Maintenance is affected","Elect. Mach. & Equip.","General Appearance","Equipment Related","11.4","Very High","","","Requisition was recd, Spares recd on 26 Aug 2020, but only for Filter, other spares still awaiting. Deck air comp made operational , will pick up pending spares in msgs .","2020-09-30","Req No : ZENO200043","Completed","2020-09-07","No","No","No","Internal"]
[null,null,null,null,13747,"36_2 Sep 2020 12:23:57 PM","2020-08-05","Defect","Ship Staff","Ship Staff Insp.","Stbd Gangway Winch Motor : Observed not working","Deck - Machinery","Safety / LSA / FFA","Equipment Related","5.47","Medium","","","Motor Overhauled & Tested, working satisfactory","2020-08-31","","Completed","2020-08-08","No","No","No","Internal"]
[null,null,null,null,13748,"36_2 Sep 2020 12:27:37 PM","2020-08-05","Defect","Ship Staff","Ship Staff Insp.","Filter Assembly of Stbd Pilot Ladder Motor : Observed wasted, protection cover also wasted","Deck - Machinery","Safety / LSA / FFA","Equipment Related","5.47","Medium","","","Fabricated new protection cover, fixed new recd filter assembly, tested, found satidfactory","2020-08-31","","Completed","2020-08-12","No","No","No","Internal"]
[null,null,null,null,13749,"36_2 Sep 2020 12:39:10 PM","2020-08-05","Defect","Ship Staff","Ship Staff Insp.","Fire Hose Box : Outside Paint Room, Observed Securing Arrangemnt was broken","LSA / FFA","Safety / LSA / FFA","External Factors","","","","","Repaired, good condition","2020-08-12","","Completed","2020-08-12","No","No","No","Internal"]
[null,null,null,null,13750,"36_2 Sep 2020 12:41:20 PM","2020-08-05","Defect","Ship Staff","Ship Staff Insp.","Securing Box of Cable for Stbd Lifeboat was observed broken","LSA / FFA","Safety / LSA / FFA","External Factors","5.29","High","","","Door repaired, fixed back. Good condition","2020-08-13","","Completed","2020-08-12","No","No","No","Internal"]
[null,null,null,null,13738,"36_2 Sep 2020 10:31:42 AM","2020-08-06","Breakdown,Critical Equipment","Ship Staff","Ship Staff Insp.","Observed Deep Groove on Stopper Bar of Stbd Anchor","Deck - Mooring Machinery","Mooring","Equipment Related","9.2","Very High","","","Groove needs to be filled up either in Dry Dock OR onboard by Dismantling & carrying to E/R for Filling, VERY HEAVY EQUIPMENT","2020-10-17","","Completed","2020-10-17","No","No","No","Internal","Job completed on board by ship staff."]
[null,null,null,null,13751,"36_2 Sep 2020 12:31:27 PM","2020-08-06","Defect","Ship Staff","Ship Staff Insp.","Various Air Leaks on Deck (Bridge Deck Stbd, Pumproom Top/stbd/ Upper deck/stbd)","Deck - Machinery","Structural Condn. / WT integrity ","External Factors","","","","","Bridge Deck/stbd : Applied Putty, Pumproom top/stbd : New pipe fabricated & fixed, Upper deck/stbd : New valve fixed","2020-08-31","","Completed","2020-08-19","No","No","No","Internal"]
[null,null,null,null,13752,"36_2 Sep 2020 12:35:45 PM","2020-08-06","Defect","Ship Staff","Ship Staff Insp.","Stripper Pump Gland Packing : Observed Leaking","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.8","Medium","","","Gland Packing renewed, leak arretsed","2020-08-11","","Completed","2020-08-07","No","No","No","Internal"]
[null,null,null,null,13753,"36_2 Sep 2020 12:49:44 PM","2020-08-06","Defect","Ship Staff","Ship Staff Insp.","Port HHC : Oil Leak Observed on pipe & valve","Deck - Machinery","Structural Condn. / WT integrity ","Equipment Related","8.63","High","","","New pipe (copper) fabricated, valve repaired, fixed back & tested, leak arrested, working good","2020-08-13","","Completed","2020-08-07","No","No","No","Internal"]
[null,null,null,null,13567,"36_15 Aug 2020 8:53:25 AM","2020-08-06","Critical Equipment","Ship Staff","Ship Staff Insp.","Emergency Generator Batteries indication found in white instead of green while in continuous charging mode.","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","new baterries recieved and installed.","2020-08-18","ZENO200151","Completed","2020-08-28","No","No","No","Internal","Spares arranged by Owners.  Was this supplied on board at S'pore on 26082020?"]
[null,null,null,null,13568,"36_15 Aug 2020 7:55:25 AM","2020-08-07","Critical Equipment","Ship Staff","Ship Staff Insp.","Emergency Generator hydraulic starter not working.","Critical Equip.","Emgcy. Systems","Equipment Related","11.4","Very High","","","spares recieved and installed, now hand pump working satisfactory.","2020-11-30","ZENO200098","Completed","2020-12-27","No","No","No","Internal","Understand partial spares were supplied on board on 26082020 @ S'pore.  The balanced still pending."]
[null,null,null,null,13569,"36_15 Aug 2020 8:01:25 AM","2020-08-10","Observation","Ship Staff","Ship Staff Insp.","No spares/consumables available for ME fuel pump overhauling","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","spares recieved","2020-08-18","ZENO200069","Completed","2020-08-26","No","No","No","Internal","Spares should have been supplied on board @ S'pore on 26082020"]
[null,null,null,null,13740,"36_3/9/2020 10:01:25 AM","2020-08-16","Defect","Ship Staff","Ship Staff Insp.","COPT Vacuum condenser safety disc burst due to defect in the disc.","Cargo Mach.","Eng. / Strg. Comp.","Equipment Related","8.2","Medium","","","Bursting disc renewed from spare.RO raised - ZENO200169 for a spare disc. ","2020-08-16","ZENO200169","Completed","2020-08-16","No","No","No","Internal","We have closed-out this defect in DDRL since the spares were received & defect rectified in the initial stage. For the bursting of disc in August 2020, please create another defect record for same."]
[null,null,null,null,13745,"36_2 Sep 2020 11:42:45 AM","2020-08-24","Critical Equipment","Ship Staff","Ship Staff Insp.","15 PPM unit behaviour is erratic","Critical Equip.","Eng. / Strg. Comp.","Equipment Related","6.3","Low","","","Unit calibrated by shore technician and display unit's defective components were replaced. System tested, found satisfactory.","2020-11-20","","Completed","2020-10-28","No","No","No","Internal","The target already overdue and new / reconditioned cell supplied on 26th Aug 2020  but to date, we are still awaiting on outcome of your fault finding."]
[null,null,null,null,13746,"36_2 Sep 2020 11:18:02 AM","2020-08-25","Defect","Ship Staff","Ship Staff Insp.","Valve : Observed 2S WB valve indicator on CCR Panel is showing shut, Valve is opening & closing 100% propely. Indicator is faulty","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.21","High","","","Potentiometer found defective and renewed. Spare will be ordered.","2020-11-30","","Completed","2020-09-15","No","No","No","Internal","Pls revert with update on progress status?"]
[null,null,null,null,13743,"36_2 Sep 2020 11:03:56 AM","2020-08-26","Defect","Ship Staff","Ship Staff Insp.","Observed 1Stbd COT IG Pressure Sensor not working","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.19","High","","","Spare recd & fixed, working good.","2020-11-26","ZENO200181","Completed","2020-10-25","No","No","No","Internal","Awaiting approval from Owner, sent on 25th Sept 2020"]
[null,null,null,null,13754,"36_2 Sep 2020 12:44:04 PM","2020-08-26","Defect","Ship Staff","Ship Staff Insp.","PV Breaker Vent valve : Observed not operating properly","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.28","Medium","","","Valve repaired & fixed back, operated, found working good","2020-08-31","","Completed","2020-08-27","No","No","No","Internal"]
[null,null,null,null,17371,"36_15/1/2021 5:42:50 PM","2020-08-26","Defect","Ship Staff","Ship Staff Insp.","NO.1 COP EMERGENCY STOP ERRATIC / UNRELIABLE AS REPORTED – TO CHECK/ TROUBLESHOOT AND ADVISE FINDING","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.1","Very High","","","COP trip connections and wiring chkd, Tried out and working satisfactory from all places. ","2020-10-10","","Completed","2020-09-18","No","No","No","Internal"]
[null,null,null,null,17372,"36_15/1/2021 5:45:49 PM","2020-08-26","Observation","Ship Staff","Ship Staff Insp.","WBT TANK ULLAGE/SOUNDING REQUIRES TO BE PURGED VERY OFTEN – TO INVESTIGATE AND ADVISE FINDING","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.12","Medium","","","Problem rectified.","2020-10-25","","Completed","2020-10-20","No","No","No","Internal"]
[null,null,null,null,17373,"36_15/1/2021 5:48:31 PM","2020-08-26","Observation","Ship Staff","Ship Staff Insp.","NO.1 AVSS CCR INDICATION ERROR – INVESTIGATE AND ADVISE/ REPAIR","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.8","Medium","","","On Investigation, observed the Separator Level Valve on Top side of the Separator was “Full Shut”. Same has been opened. Working good.","2020-10-10","","Completed","2020-10-10","No","No","No","Internal"]
[null,null,null,null,17374,"36_15/1/2021 6:03:29 PM","2020-08-26","Observation","Ship Staff","Ship Staff Insp.","FORWARD EDUCTOR (FORECASTLE STORE) TO TRY OUT","Deck - Machinery","MARPOL Related","Equipment Related","6.1","Medium","","","Tried out, Working Satisfactory, Seals Renewed & Logged","2020-09-25","","Completed","2020-09-07","No","No","No","Internal"]
[null,null,null,null,17375,"36_15/1/2021 6:06:20 PM","2020-08-26","Observation","Ship Staff","Ship Staff Insp.","ICCP – ANODE AMPS SHOWING MINUS ZERO – TO INVESTIGATE AND ADVISE.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","ICCP Fwd unit is slave mode and engine room unit Master as easier to monitor. Master unit controls and shows correct Amps, Slave unit shows Amp as 0 .","2020-10-10","","Completed","2020-09-22","No","No","No","Internal"]
[null,null,null,null,17376,"36_15/1/2021 6:08:40 PM","2020-08-26","Observation","Ship Staff","Ship Staff Insp.","SOME AREAS ON DECK – SURFACE PREPARATION NOT DONE PROPERLY – DISCUSSED WITH CO","Deck - Pipe / Fittings","General Appearance","Inappropriate Procedure","11.3","Medium","","","Noted : Some Previously done areas were not prepared correctly, Currently care is being taken about Surface Preparation","2020-11-25","","Completed","2020-09-07","No","No","No","Internal"]
[null,null,null,null,17377,"36_15/1/2021 5:58:42 PM","2020-08-26","Observation","Ship Staff","Ship Staff Insp.","PV BREAKER VENT VALVE TO RENEW","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","12.19","High","","","Valve renewed.","2020-09-25","","Completed","2020-08-27","No","No","No","Internal"]
[null,null,null,null,17378,"36_15/1/2021 5:53:49 PM","2020-08-26","Observation","Ship Staff","Ship Staff Insp.","SOME DRESSER COUPLING (AS DISCUSSED WITH CO) STUDS CORRODED. TO PLAN AND RENEW AS NECESSARY","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","11.5","Medium","","","Studs replaced as required. Dessor coupling in good condition.","2020-11-25","","Completed","2020-11-25","No","No","No","Internal"]
[null,null,null,null,17379,"36_15/1/2021 5:56:35 PM","2020-08-26","Observation","Ship Staff","Ship Staff Insp.","MOT LADDER WHEELS SIEZED – SAME TO FREE","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","11.5","Medium","","","Completed (MOT & Securing Clamp Areas Spot Derusted/painted, Securing Wires Renewed, Wheels Derusted/painted & made free)\n\n","2020-11-28","","Completed","2020-09-11","No","No","No","Internal"]
[null,null,null,null,14039,"36_14/09/2020 16:41:10","2020-08-28","Observation","Ship Staff","Nav Audit / Verification","Anemometer Dimmer Found Not Working","Navigation - Others","Navigation","Equipment Related","4.7","High","","","Spares recieved, job completed.","2020-11-28","","Completed","2020-10-28","No","No","No","Internal","Please revert with updated status on progress of repairs on 2nd attempt."]
[null,null,null,null,14042,"36_14/09/2020 16:47:12","2020-08-28","Non Conformity","Ship Staff","Nav Audit / Verification","Loud Hailer Found Defective","Navigation - Others","Navigation","Equipment Related","","","","","New Batteries Intsalled in Loud Hailer Were Found to be drained out , Another Set of New batteries were Fitted and Loud Hailer was Found Working Satisfactory.","2020-11-28","","Completed","2020-09-09","No","No","No","Internal"]
[null,null,null,null,14043,"36_14/09/2020 16:51:18","2020-08-28","Non Conformity","Ship Staff","Nav Audit / Verification","Manovering Booklet Hard Copy Not available on bridge ","Navigation - Others","Navigation","Inappropriate Procedure","","","","","Hard Copy Of Manovering Booklet was printed out from Manual /Soft Copy and Same placed near  Engine Console Panel On Bridge ","2020-11-28","","Completed","2020-09-09","No","No","No","Internal"]
[null,null,null,null,13744,"36_2 Sep 2020 11:47:06 AM","2020-08-30","Defect","Ship Staff","Ship Staff Insp.","Both Aux boilers have high load fluctuations , during discharging , even if the COPT load is stable.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","11.4","Very High","","","Calibrated all pressure transducers and cleared all capillary lines. Now boilers are operating steadily.","2020-11-30","","Completed","2020-10-26","No","No","No","Internal","Target date overdue but to date office is still awaiting update of any progress in the fault finding."]
[null,null,null,null,14044,"36_15 Sep 2020 2:56:19 AM","2020-09-04","Defect","Ship Staff","Ship Staff Insp.","Observed Flow Fail Alarm on !S WBT Gas Detection Sysyem Line","Hull & Tanks","Cargo / Ballast Systems","Equipment Related","5.21","Medium","","","Renewed Flame Arrestor in CCR Cabinet, tested, working satisfactory","2020-09-15","","Completed","2020-09-07","No","No","No","Internal"]
[null,null,null,null,14041,"36_15 Sep 2020 9:39:10 AM","2020-09-15","Critical Equipment","Ship Staff","Ship Staff Insp.","Fire Detection system unable to detect smoke detector for Gymnasium","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.39","Very High","","","System repaired by shore technician on 28th Oct.System tested, working satisfactory.","2020-10-31","","Completed","2020-10-28","No","No","No","Internal","Technical Supt. to update vessel on shore/technician assistance required."]
[null,null,null,null,14241,"36_30 Sep 2020 8:35:33 AM","2020-09-29","Breakdown","Ship Staff","Ship Staff Insp.","IG Pressure Sensor for 6P COT Malfunctioned on 29 Sep 20.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.19","High","","","Recd Spare, fixed, working good","2020-11-30","ZENO200181","Completed","2020-10-25","No","No","No","Internal","Sent to Owner for approval on 25th Sept. 2020"]
[null,null,null,null,14874,"36_19 Oct 2020 11:25:59 AM","2020-10-19","Defect","Ship Staff","Ship Staff Insp.","Vacuum Condenser bursting disc imploded towards vacuum.","Cargo Mach.,E/R - Boiler","Cargo / Ballast Systems","Equipment Related","11.4","Very High","","","Spares recieved, job completed.","2020-11-30","ZENO200169","Completed","2020-12-28","No","No","No","Internal","Based on VFF, the order was supplied on board on 19th Dec 2020 @ Singapore.  Please revert with updated status for said defect."]
[null,null,null,null,14873,"36_20 Oct 2020 8:42:31 AM","2020-10-28","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","VECS O2 Sensor giving low-flow alarm","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.33","Medium","","","Filter was cleaned on board,  fixed back, low-flow alarm gone. Requisition raised for spare Filter & O2 Sensor","2021-01-30","ZENO200227","Completed","2020-11-05","No","No","No","Internal",""]
[null,null,null,null,16814,"36_6 Jan 2021 12:34:26 PM","2020-10-28","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Bilge Fire and GS Pump mechanical seal found leaking. Same to be renewed.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.31","Very High","","","Presently both Fire and GS pump has no mechanical seal  leakage.","2021-01-31","","Completed","2021-01-14","No","No","No","Internal"]
[null,null,null,null,16816,"36_6/1/2021 2:42:37 PM","2020-10-28","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Area below bridge wing and accommodation block paint is peeling off. To be de-rusted and painted.","Accommodation","General Appearance","Equipment Related","11.8","Low","","","Derusting & Painting of the Bridge wing & accomodation Block carried.","2021-01-27","","Completed","2021-01-27","No","No","No","Internal"]
[null,null,null,null,16818,"36_6/1/2021 2:55:20 PM","2020-10-28","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Stbd Side manifold area between No. 2 and No. 3 / No. 1 and No. 3 manifolds the chequered plates to be renewed as same is holed.","Hull & Tanks","Structural Condn. / WT integrity ","Equipment Related","11.5","Medium","","","Chequered plates fabricated & fitted at location to ensures holes are covered.","2021-01-27","","Completed","2021-01-27","No","No","No","Internal"]
[null,null,null,null,16826,"36_30 Dec 2020 10:27:23 AM","2020-10-28","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ECR Panels are dirty and dusty. To be cleaned.","Elect. Mach. & Equip.","General Appearance","Equipment Related","11.1","High","","","ECR Panels are cleaned.","2020-11-15","","Completed","2020-11-15","No","No","No","Internal"]
[null,null,null,null,16827,"36_30 Dec 2020 12:13:46 PM","2020-10-28","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Both Steering gear Jenney pumps were found with slight leaks. Same to be rectified by renewing the seals.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.39","High","","","Both Steering gear Jenney oil seals renewed.","2020-12-30","","Completed","2020-12-18","No","No","No","Internal"]
[null,null,null,null,16828,"36_30 Dec 2020 12:16:40 PM","2020-10-28","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Electrical panels are dirty from the top and outside. To be cleaned on priority.","Elect. Mach. & Equip.","General Appearance","Equipment Related","10.37","Medium","","","All Electrical panels are  cleaned .","2020-11-15","","Completed","2020-11-10","No","No","No","Internal"]
[null,null,null,null,16829,"36_30 Dec 2020 12:19:06 PM","2020-10-28","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","No. 2 AE Unit 4 exhaust pyrometer not working. To be renewed.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","No. 2 AE Unit 4 exhaust pyrometer  renewed.","2020-11-15","","Completed","2020-11-03","No","No","No","Internal"]
[null,null,null,null,16830,"36_30 Dec 2020 12:22:14 PM","2020-10-28","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","All generators top including the turbocharger areas to be cleaned thoroughly.","E/R - Aux. Engine","General Appearance","Equipment Related","10.32","Very High","","","All generators top including the turbocharger areas cleaned thoroughly.","2020-11-30","","Completed","2020-11-22","No","No","No","Internal"]
[null,null,null,null,16831,"36_30 Dec 2020 12:25:34 PM","2020-10-28","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","MGO FW Cooler to be tried out.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","MGO FW Cooler tried out.","2020-11-15","","Completed","2020-11-04","No","No","No","Internal"]
[null,null,null,null,16832,"36_30 Dec 2020 12:27:25 PM","2020-10-28","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","The observation tank to be cleaned thoroughly. ","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","The observation tank cleaned thoroughly. ","2020-11-15","","Completed","2020-11-01","No","No","No","Internal"]
[null,null,null,null,16833,"36_30 Dec 2020 2:10:03 PM","2020-10-28","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Last cleaning dates are not stencilled on the condensers and heat exchangers. To be done.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.1","Medium","","","Last cleaning dates are stencilled on the condensers and heat exchangers.","2020-11-15","","Completed","2020-11-07","No","No","No","Internal"]
[null,null,null,null,16834,"36_30 Dec 2020 2:15:48 PM","2020-10-28","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","HFO Overflow slight glass found dirty. Same to be cleaned. ","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","HFO Overflow slight glass cleaned. ","2020-11-15","","Completed","2020-11-10","No","No","No","Internal"]
[null,null,null,null,16835,"36_30 Dec 2020 2:17:42 PM","2020-10-28","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Bilge Fire and GS Pump pipe connection to GS line section found leaking. Same to be renewed.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Bilge Fire and GS Pump pipe connection to GS line section found leaking. Same renewed.","2020-11-15","","Completed","2020-10-31","No","No","No","Internal"]
[null,null,null,null,16836,"36_30 Dec 2020 2:20:11 PM","2020-10-28","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Traces of leaks found on the stern tube fwd seal. Same to be included in Refman for rectification during the next docking related repairs. ","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Job included in Refman for rectification during the next docking related repairs. ","2020-12-31","","Completed","2020-12-20","No","No","No","Internal"]
[null,null,null,null,16837,"36_30 Dec 2020 2:23:14 PM","2020-10-28","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","No. 2 Aux Boiler Steam outlet valve found leaking from the gland. To be rectified.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","No. 2 Aux Boiler Steam outlet valve gland  leak rectified.","2020-11-15","","Completed","2020-11-05","No","No","No","Internal"]
[null,null,null,null,16838,"36_30 Dec 2020 8:25:21 PM","2020-10-28","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Vessel does not have a spare new liner. Requisition for the same to be raised.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.1","Medium","","","Requisition raised for a main engine spare liner.","2020-11-15","ZENO200235","Completed","2020-11-02","No","No","No","Internal"]
[null,null,null,null,16839,"36_30 Dec 2020 8:27:45 PM","2020-10-28","Breakdown","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Railing broken near engine room casing to the funnel deck. To be rectified.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Railing broken near engine room casing rectified.","2020-11-15","","Completed","2020-11-03","No","No","No","Internal"]
[null,null,null,null,16840,"36_30 Dec 2020 8:30:49 PM","2020-10-28","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Found port side drain on the funnel top chocked. To be cleared. ","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","",""," Chocked drain for port side  funnel top cleared. ","2020-11-15","","Completed","2020-11-10","No","No","No","Internal"]
[null,null,null,null,16841,"36_30 Dec 2020 12:29:48 PM","2020-10-28","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Hot well tank covers securing pins are missing. To be repaired. ","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Hot well tank covers securing pins repaired. ","2020-11-15","","Completed","2020-11-01","No","No","No","Internal"]
[null,null,null,null,16842,"36_30 Dec 2020 8:33:10 PM","2020-10-28","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Aux. Boiler panel doors are not closing properly. Same to be repaired on an URGENT basis. ","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Aux. Boiler panel doors repaired.","2020-11-15","","Completed","2020-11-02","No","No","No","Internal"]
[null,null,null,null,16843,"36_30 Dec 2020 8:35:39 PM","2020-10-28","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Deck Air compressor efficiency is poor. To be investigated and rectified. ","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Deck Air compressor efficiency is poor. To be investigated and rectified. ","2020-11-15","","Completed","2020-11-01","No","No","No","Internal"]
[null,null,null,null,16844,"36_1 Jan 2021 8:30:48 AM","2020-10-28","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Forecastle store needs proper soap wash and cleaning and needs to be rearranged. The electrical panels and the solenoid valves are to be cleaned of dust. The bulkheads needs to be cleaned. ","Miscellaneous","General Appearance","Equipment Related","11.12","Low","","","CLEANING JOB COMPLETED.","2020-11-28","","Completed","2020-11-20","No","No","No","Internal"]
[null,null,null,null,17356,"36_15/1/2021 6:42:33 PM","2020-10-28","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Steam WBP bearing temp gauge is defective. Spares on order. Same to be replaced when spares received on board.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","Steam WBP bearing temp gauge replaced with new spare. Tried out and found  working satisfactory.","2021-01-27","","Completed","2021-01-08","No","No","No","Internal"]
[null,null,null,null,16845,"36_1/1/2021 11:04:42 AM","2020-10-28","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","No. 1 Stbd Tank COW Root valve is in poor condition. To be overhauled.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.34","High","","","Overhauling of the valve carried out.","2020-11-28","","Completed","2020-11-19","No","No","No","Internal"]
[null,null,null,null,17357,"36_15/01/2021 20:39:07","2020-10-28","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Deck Seal Low Flow sendor defective and bypassed. Spare on order. Same to be replaced when spares received onboard","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","11.4","Very High","","","Deck seal low flow sensor removed, cleaned and put back. Tried out found satisfactory","2021-01-28","","Completed","2021-01-20","No","No","No","Internal"]
[null,null,null,null,16846,"36_1/1/2021 11:12:33 AM","2020-10-28","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Port side hose handling crane Manhole door 3 bolt holes found missing. To be renewed. ","Deck - Machinery","Structural Condn. / WT integrity ","Equipment Related","8.5","Very High","","","Bolts put in place on the manhole.","2020-11-28","","Completed","2020-12-14","No","No","No","Internal"]
[null,null,null,null,16847,"36_1/1/2021 11:18:51 AM","2020-10-28","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Wilden pumps used for SOPEP have a cracked casing. To be repaired.","Deck - Machinery,Miscellaneous","Cargo / Ballast Systems","Equipment Related","6.3","Low","","","Repaired and operation checked.","2020-11-28","","Completed","2020-11-15","No","No","No","Internal"]
[null,null,null,null,16848,"36_1/1/2021 11:23:21 AM","2020-10-28","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Poop deck Stbd side Aft winch M5 and M6 inlet lines to be renewed. Rusted bolts to be renewed.","Deck - Mooring Machinery","Mooring","Equipment Related","9.14","Medium","","","Derusting and painting carried out. ","2021-01-27","","Completed","2020-12-11","No","No","No","Internal"]
[null,null,null,null,16849,"36_1/1/2021 11:29:27 AM","2020-10-28","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","1 Stbd COT Cargo tank pressure sensor is still erratic are renewal of sensor due to possible faulty cable. Same to be investigated and rectified.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.19","High","","","Sensor cable renewed. Operation satisfactory.","2020-11-27","","Completed","2020-11-20","No","No","No","Internal"]
[null,null,null,null,16850,"36_1/1/2021 12:34:11 PM","2020-10-28","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Load testing of all loose lifting gear overdue. Load cell supplied to the vessel at Singapore and all loose gear load test to be completed and equipment tagged.","Miscellaneous","Cert. & Docu.","Equipment Related","8.5","Very High","","","Load test of all the loose lifting gear carried out.","2020-11-27","","Completed","2020-11-17","No","No","No","Internal"]
[null,null,null,null,16851,"36_1/1/2021 12:39:36 PM","2020-10-28","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","No means available on board to download the data from the VDR so that the same can be reviewed on board. Suitable arrangements to be put into place. ","Navigation - VDR / BNWAS","Navigation","Equipment Related","4.11","Medium","","","Troubleshooting Carried out with maker. For downloading data technician will be required always because limitation of firewire cable connection. Email dated 11.11.2020 from Mr Kamlesh Solanki","2020-12-27","","Completed","2020-11-11","No","No","No","Internal"]
[null,null,null,null,16852,"36_1/1/2021 12:47:13 PM","2020-10-28","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Bridge officers to check regarding SNR / RMS values as same noted as done in the change of watch checklist.","Documentation","Navigation","Inappropriate Procedure","4.3","Medium","","","SNR Value Checked for Satellite being Tracked , As per the Maker Manual SNR to be more than 32 , Vessel GPS complying with requirement, All Duty Officer Explained the Procedure for Checkling the SNR value , Vessel Complying with Change over watch checklist 12.01.35.041.02","2020-11-12","","Completed","2020-10-30","No","No","No","Internal"]
[null,null,null,null,16853,"36_1/1/2021 12:51:04 PM","2020-10-28","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","PV Valve Flame Screens heavily rusted. Same to be replaced with spare screen provided at Singapore.","Hull & Tanks","Cargo / Ballast Systems","Equipment Related","8.4","Medium","","","PV Valve flame screens renewed.","2020-12-27","","Completed","2020-12-08","No","No","No","Internal"]
[null,null,null,null,16854,"36_1/1/2021 12:55:01 PM","2020-10-28","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Holding frame for Vacuum side of PV valve is cracked and wasted. Same to be repaired by welding.","Hull & Tanks","Cargo / Ballast Systems","Equipment Related","8.4","Medium","","","Holding frame for Vacuum side of PV valve removed from location, welded and fitted back in position. ","2020-12-27","","Completed","2020-12-08","No","No","No","Internal"]
[null,null,null,null,16855,"36_5/1/2021 1:46:12 PM","2020-10-28","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Stbd side pump room bilges are dirty. To be cleaned and painted.","Miscellaneous","General Appearance","Equipment Related","8.44","High","","","Bilges cleaned.","2021-01-27","","Completed","2021-01-04","No","No","No","Internal"]
[null,null,null,null,16856,"36_6 Jan 2021 12:18:42 PM","2020-10-28","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","No. 3 AE No 5 JCW temp gauge not working. To be renewed. ","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","No. 3 AE No 5 JCW temp gauge replaced.","2021-01-10","","Completed","2020-12-29","No","No","No","Internal"]
[null,null,null,null,16857,"36_1/1/2021 12:42:38 PM","2020-10-28","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Entries for weekly and monthly check of SART, EPIRB, L/B VHF radios etc. not signed by concerned officer in the GMDSS Logbook. ","Documentation","Navigation","Inappropriate Procedure","4.23","High","","","Entries Signed By Concerned officer in GMDSS Log Book","2020-11-27","","Completed","2020-10-29","No","No","No","Internal"]
[null,null,null,null,17380,"36_15/1/2021 6:39:53 PM","2020-10-28","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Numerous lights around the vessel found fused or missing due to no stock. New stock has been supplied at Singapore and fused lights to be replaced on priority.","Elect. Mach. & Equip.","General Appearance","Equipment Related","","","","","FUSED LIGHTS REPLACEMENT JOB COMPLETED","2020-11-27","","Completed","2020-11-09","No","No","No","Internal"]
[null,null,null,null,null,"36_15/1/2021 6:36:32 PM","2020-12-20","Observation","Ship Staff","Nav Audit / Verification","On stbd Bridge Wing, Dimmer of  Rudder Angle Indicator repeater not Operational.","Navigation - Others","Navigation","Equipment Related","4.7.19","High","Not Applicable","Not Applicable","Dimmer for Rudder angle indicator on Stbd Bridge Wing was opened & checked , it was noted that the illumination light plate was burned & not  Working , Requisition for the Same was raised ZENO210005. requsition recieved and fault rectified.","2021-03-20","ZENO210005","Completed","2021-06-10","No",null,null,"Internal"]
[null,null,null,null,null,"36_31/3/2021 5:44:09 PM","2021-02-25","Defect","Ship Staff","Ship Staff Insp.","Provision crane port high pressure line parted from adpator.","Deck - Machinery","Eng. / Strg. Comp.","Equipment Related",8.76,"Medium","Not Applicable","Not Applicable","High pressure line to be replaced.","2021-02-25",null,"Completed","2021-02-25","No",null,null,"Internal"]
[null,null,null,null,null,"36_22/3/2021 2:14:52 PM","2021-02-25","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","The Tank Cleaning Machines & Hoses current condition.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related",8.6300000000000008,"High","Not Applicable","Not Applicable","Hand cranking of all COW machines and visual inspection of drive unit carried out  & found Satisfactory. Portable hoses are tagged with condemn / do not use by by previous management and does not have certificates for these hoses, overall condition of these hoses is not good and is unusable.","2021-05-31",null,"Completed","2021-05-31","No",null,null,"Internal"]
[null,null,null,null,null,"36_22/3/2021 3:00:48 PM","2021-02-25","Observation","Ship Staff","Ship Staff Insp.","Vessel has only 1 UTI's - Gastight Operational.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related",8.1199999999999992,"Medium","Not Applicable","Not Applicable","Vessel received 3 Restricted UTI + 1 Gas Tight UTI at Lome on 08th May 2021. ","2021-05-25",null,"Completed","2021-05-08","No",null,null,"Internal"]
[null,null,null,null,null,"36_28/3/2021 3:32:34 PM","2021-02-25","Defect","Ship Staff","Ship Staff Insp.","VHF No.2 Handset cable faulty.","Navigation - Others","Navigation","Equipment Related",4.7,"High","Not Applicable","Not Applicable","Requisition  ZENO210039 received, new handset connected to the VHF and is in good working condition.","2021-05-25",null,"Completed","2021-05-30","No",null,null,"Internal"]
[null,null,null,null,null,"36_30/3/2021 4:23:31 PM","2021-03-10","Critical Equipment","Ship Staff","Ship Staff Insp.","Emergency generator hydraulic hand pump is taking longer to develop pressure.","Critical Equip.","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Hydraulic hand pump to be overhauled.","2021-03-11",null,"Completed","2021-03-11","No",null,null,"Internal"]
[null,null,null,null,null,"36_28 Mar 2021 5:08:52 PM","2021-03-15","Defect","Ship Staff","Ship Staff Insp.","Fresh water generator dosing pump is not efficient","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Dosing pump to be inspected and hoses to be cleared.","2021-03-20",null,"Completed","2021-03-17","No",null,null,"Internal"]
[null,null,null,null,null,"36_28/3/2021 3:47:51 PM","2021-03-17","Defect","Ship Staff","Ship Staff Insp.","Cascade tank level gauge is opaque","Miscellaneous","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Sight glass to be renewed.","2021-03-22",null,"Completed","2021-03-19","No",null,null,"Internal"]
[null,null,null,null,null,"36_28 Mar 2021 5:26:26 PM","2021-03-18","Defect","Ship Staff","Ship Staff Insp.","Aux engine number 1 local stop push button malfunctioning","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Local push button to inspect cleaned and renew if reqired.","2021-03-25",null,"Completed","2021-03-20","No",null,null,"Internal"]
[null,null,null,null,null,"36_30/3/2021 4:08:42 PM","2021-03-18","Defect","Ship Staff","Ship Staff Insp.","Sludge pump filter not in good condition.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Sludge pump filter inside mesh to be renewed.","2021-03-20",null,"Completed","2021-03-19","No",null,null,"Internal"]
[null,null,null,null,null,"36_30/3/2021 4:50:53 PM","2021-03-22","Defect","Ship Staff","Ship Staff Insp.","Aux engine no 1 local stop button malfunctioning.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Local stop button to be inspected and repaired.","2021-03-25",null,"Completed","2021-03-23","No",null,null,"Internal"]
[null,null,null,null,null,"36_28/3/2021 3:10:32 PM","2021-03-28","Defect","Ship Staff","Ship Staff Insp.","Main engine loop fail alarm is active on Safety system unit","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","PCB to be renewed.","2021-05-30","ZENO210032","Completed","2021-06-09","No",null,null,"Internal"]
[null,null,null,null,null,"36_28/3/2021 3:13:21 PM","2021-03-28","Defect","Ship Staff","Ship Staff Insp.","Deck air compressor inoperational","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Motor and pulley to be renewed.","2021-05-30","ZENO210012","Completed","2021-06-09","No",null,null,"Internal"]
[null,null,null,null,null,"36_28/3/2021 3:35:53 PM","2021-03-28","Defect","Ship Staff","Ship Staff Insp.","Navigation indicator panel lights are not working","Navigation - Others","Navigation","Equipment Related",4.8,"Medium","Not Applicable","Not Applicable","Req ZENO210030 recieved and fault rectified.","2021-03-30","ZENO210030","Completed","2021-06-04","No",null,null,"Internal"]
[null,null,null,null,null,"36_28/3/2021 3:39:06 PM","2021-03-28","Defect","Ship Staff","Ship Staff Insp.","Bridge anemometer illumination light is not working","Navigation - Others","Navigation","Equipment Related",4.8,"Medium","Not Applicable","Not Applicable","ZENO210036 recieved fault rectified.","2021-05-30","ZENO210036","Completed","2021-06-03","No",null,null,"Internal"]
[null,null,null,null,null,"36_30/3/2021 5:09:56 PM","2021-03-30","Defect","Ship Staff","Ship Staff Insp.","Incinerator dosing pump bearings to renew.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Incinerator dosing pump bearings to be renewed.","2021-04-30",null,"Completed","2021-04-01","No",null,null,"Internal"]
[null,null,null,null,null,"36_30/3/2021 5:26:26 PM","2021-03-30","Defect","Ship Staff","Ship Staff Insp.","Main engine FO oil circulating pump mechanical seal is leaking.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Mechanical seal to be renewed.","2021-05-30",null,"Completed","2021-04-15","No",null,null,"Internal"]
[null,null,null,null,null,"36_30/3/2021 5:34:16 PM","2021-03-30","Defect","Ship Staff","Ship Staff Insp.","Aux engine FO booster pump no. 1 mechanical seal is leaking.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Mechanical seal to be replaced.","2021-05-30","ZENO210071","Completed","2021-06-09","No",null,null,"Internal"]
[null,null,null,null,null,"36_31/3/2021 9:14:06 AM","2021-03-31","Defect","Ship Staff","Ship Staff Insp.","MGPS of high sea chest is not working.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related",10.31,"Very High","Not Applicable","Not Applicable","MGPS trnasformer and transistor to be replaced.","2021-05-30","ZENO210001","Completed","2021-06-08","No",null,null,"Internal"]
[null,null,null,null,null,"36_31/3/2021 5:49:04 PM","2021-03-31","Defect","Ship Staff","Ship Staff Insp.","3 nos Laundry dryers are not working.","Miscellaneous","MLC Related","Equipment Related",null,null,"Not Applicable","Not Applicable","Dryers to be replaced.","2021-05-30","ZENO210062","Completed","2021-05-31","No",null,null,"Internal"]
[null,null,null,null,null,"36_31/3/2021 5:52:26 PM","2021-03-31","Defect","Ship Staff","Ship Staff Insp.","4 hot plates in galley are not working.","Miscellaneous","MLC Related","Equipment Related",null,null,"Not Applicable","Not Applicable","Hot plates to be renewed.","2021-05-30","ZENO210007","Completed","2021-05-12","No",null,null,"Internal"]
[null,null,null,null,null,"36_8/5/2021 5:12:11 PM","2021-04-19","Non Conformity","Ship Staff","Cargo Audit","NAPA - Loadicator License Expired","Miscellaneous","Cargo / Ballast Systems","Equipment Related",8.6999999999999993,"High","Not Applicable","Not Applicable","Loadicator License to be  Renewed.","2021-07-19","Office Notified.","Completed","2021-04-29","No",null,null,"Internal"]

{"sheet":"Calc","index":2,"n_rows":28,"n_cols":12,"rows_kept":28,"cut":false,"hidden":true,"merged":[]}
["Def_type","Def_cause","Equipments","VIQrefno","Observer_code"]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,"Dim itemSele As Long"]
[null,null,null,null,null,null,null,null,null,null,null,"   dim startRow as integer"]
[null,null,null,null,null,null,null,null,null,null,null,"   startRow=1"]
[null,null,null,null,null,null,null,null,null,null,null,"        For itemSele = 0 To ListBox1.ListCount - 1"]
[null,null,null,null,null,null,null,null,null,null,null,"        If ListBox1.Selected(itemSele) = True Then"]
[null,null,null,null,null,null,null,null,null,null,null,"        Worksheets(\"WorksheetName\").Range(\"A\" & startRow).Value = ListBox1.List(itemSele)"]
[null,null,null,null,null,null,null,null,null,null,null,"        startRow = startRow + 1"]
[null,null,null,null,null,null,null,null,null,null,null,"        End If"]
[null,null,null,null,null,null,null,null,null,null,null,"        Next"]
[null,null,null,null,null,null,null,null,null,null,null,"Dim LastRowA As String"]
[null,null,null,null,null,null,null,null,null,null,null,"        Dim itemSele As Long"]
[null,null,null,null,null,null,null,null,null,null,null,"       Dim startRow as integer"]
[null,null,null,null,null,null,null,null,null,null,null,"        LastRowA = ActiveSheet.Cells(Rows.count, \"A\").End(xlUp).row"]
[null,null,null,null,null,null,null,null,null,null,null,"        startQue = 0"]
[null,null,null,null,null,null,null,null,null,null,null,"        For itemSele = 0 To ListBox1.ListCount - 1"]
[null,null,null,null,null,null,null,null,null,null,null,"        For startRow = 1 To LastRowA"]
[null,null,null,null,null,null,null,null,null,null,null,"        If Worksheets(\"WorksheetName\").Range(\"A\" & startRow).Value = ListBox1.List(itemSele) Then"]
[null,null,null,null,null,null,null,null,null,null,null,"        ListBox1.Selected(itemSele) = True"]
[null,null,null,null,null,null,null,null,null,null,null,"        Exit For"]
[null,null,null,null,null,null,null,null,null,null,null,"        End If"]
[null,null,null,null,null,null,null,null,null,null,null,"        Next j"]
[null,null,null,null,null,null,null,null,null,null,null,"        Next"]
[null,null,null,null,null,null,null,null,null,null,null,"        End If"]

{"sheet":"Areaofobs","index":3,"n_rows":17,"n_cols":2,"rows_kept":17,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Cargo / Ballast Systems",11]
["Cert. & Docu.",2]
["Communication",6]
["Crew Management",3]
["Emgcy. Systems",13]
["Eng. / Strg. Comp.",14]
["General Appearance",15]
["Ice Opns.",17]
["ISM Related",7]
["ISPS Related",10]
["MARPOL Related",9]
["MLC Related",4]
["Mooring",12]
["Navigation",5]
["Safety / LSA / FFA",8]
["Structural Condn. / WT integrity ",16]

{"sheet":"Vessel_type","index":4,"n_rows":1,"n_cols":2,"rows_kept":1,"cut":false,"hidden":true,"merged":[]}
["Vessel_type","ID"]

{"sheet":"Deficiency_type","index":5,"n_rows":8,"n_cols":3,"rows_kept":8,"cut":false,"hidden":true,"merged":[]}
["TITLE","Type of deficiency_description","ID"]
["Breakdown",null,6]
["Critical Equipment",null,4]
["Defect",null,1]
["Guarantee Claim",null,8]
["Non Conformity",null,2]
["Observation",null,3]
["Other",null,7]

{"sheet":"VIQrefno","index":6,"n_rows":427,"n_cols":3,"rows_kept":427,"cut":false,"hidden":true,"merged":[]}
["VIQ_ref_no","Risk Value of observation","ID"]
["1.1","Low",8243]
["1.10","Low",8252]
["1.11","Low",8253]
["1.12","Low",8254]
["1.13","Low",8255]
["1.14","Low",8256]
["1.15","Low",8257]
["1.16","Low",8259]
["1.17","Low",8260]
["1.18","Low",8261]
["1.19","Low",8262]
["1.2","Low",8244]
["1.20","Low",8263]
["1.21","Low",8265]
["1.22","Low",8266]
["1.23","Low",8267]
["1.24","Low",8268]
["1.25","Low",8269]
["1.26","Low",8270]
["1.3","Low",8245]
["1.4","Low",8246]
["1.5","Low",8247]
["1.6","Low",8248]
["1.7","Low",8249]
["1.8","Low",8250]
["1.9","Low",8251]
["1.99","High",11258]
["10.1","Medium",8461]
["10.10","High",8470]
["10.11","Medium",8471]
["10.12","Very High",8472]
["10.13","Very High",8473]
["10.14","Medium",8474]
["10.15","Low",8475]
["10.16","Very High",8476]
["10.17","Very High",8477]
["10.18","High",8478]
["10.19","Very High",8479]
["10.2","Low",8462]
["10.20","High",8480]
["10.21","Medium",8481]
["10.22","Low",8482]
["10.23","Medium",8483]
["10.24","Low",8484]
["10.25","Very High",8485]
["10.26","High",8486]
["10.27","Medium",8487]
["10.28","Low",8488]
["10.29","Medium",8489]
["10.3","Medium",8463]
["10.30","High",8490]
["10.31","Very High",8491]
["10.32","Very High",8492]
["10.33","High",8493]
["10.34","High",8494]
["10.35","Very High",8495]
["10.36","Very High",8496]
["10.37","Medium",8497]
["10.38","Medium",8498]
["10.39","High",8499]
["10.4","High",8464]
["10.40","Medium",8500]
["10.41","Medium",8501]
["10.42","Medium",8502]
["10.43","Medium",8503]
["10.44","Medium",8504]
["10.45","Very High",8505]
["10.46","High",8506]
["10.47","Medium",8507]
["10.48","High",8508]
["10.49","Medium",8509]
["10.5","Low",8465]
["10.50","High",8510]
["10.51","Low",8511]
["10.52","Medium",8512]
["10.53","Medium",8513]
["10.54","High",8514]
["10.55","Low",8515]
["10.6","Very High",8466]
["10.7","Medium",8467]
["10.8","Medium",8468]
["10.9","Medium",8469]
["10.99","High",8516]
["11.1","High",8420]
["11.10","Medium",8429]
["11.11","Very High",8430]
["11.12","Low",8431]
["11.13","Low",8432]
["11.14","Medium",8433]
["11.15","Low",8434]
["11.16","Low",8435]
["11.17","Low",8436]
["11.2","Medium",8421]
["11.3","Medium",8422]
["11.4","Very High",8423]
["11.5","Medium",8424]
["11.6","Medium",8425]
["11.7","High",8426]
["11.8","Low",8427]
["11.9","Low",8428]
["11.99","High",8437]
["12.1","High",8438]
["12.10","High",8448]
["12.11","High",8449]
["12.12","High",8450]
["12.13","High",8451]
["12.14","High",8452]
["12.15","High",8453]
["12.16","High",8454]
["12.17","High",8455]
["12.18","High",8456]
["12.19","High",8457]
["12.2","High",8439]
["12.20","High",8458]
["12.21","High",8459]
["12.3","High",8441]
["12.4","High",8442]
["12.5","High",8443]
["12.6","High",8444]
["12.7","High",8445]
["12.8","High",8446]
["12.9","High",8447]
["12.99","High",8460]
["2.1","Very High",8296]
["2.1.9","Very High",11259]
["2.10","Medium",8304]
["2.11","Medium",8305]
["2.12","Low",8306]
["2.13","Low",8307]
["2.14","Low",8308]
["2.15","Low",8309]
["2.16","Medium",8310]
["2.2","Medium",8297]
["2.3","High",8295]
["2.4","Medium",8298]
["2.5","Medium",8299]
["2.6","Low",8300]
["2.7","High",8301]
["2.8","High",8302]
["2.9","Medium",8303]
["2.99","High",8311]
["3.1","High",8312]
["3.2","Very High",8313]
["3.3","High",8314]
["3.4","Low",8294]
["3.5","Medium",8315]
["3.6","High",8316]
["3.7","Very High",8317]
["3.8","Very High",8318]
["3.99","High",8319]
["4.1","High",8320]
["4.10","High",8329]
["4.11","Medium",8330]
["4.12","Very High",8331]
["4.13","Very High",8332]
["4.14","Very High",8333]
["4.15","Very High",8334]
["4.16","Very High",8335]
["4.17","Very High",8336]
["4.18","Very High",8337]
["4.19","Low",8338]
["4.2","Medium",8321]
["4.20","Very High",8339]
["4.21","High",8340]
["4.22","Low",8341]
["4.23","High",8342]
["4.24","High",8343]
["4.25","Low",8344]
["4.26","Low",8345]
["4.27","High",8346]
["4.3","Medium",8322]
["4.4","High",8323]
["4.5","Very High",8324]
["4.6","Medium",8325]
["4.7","High",8326]
["4.8","Medium",8327]
["4.9","Medium",8328]
["4.99","High",8347]
["5.1","Very High",8517]
["5.10","High",8526]
["5.11","Low",8527]
["5.12","Medium",8528]
["5.13","High",8529]
["5.14","Very High",8530]
["5.15","Medium",8531]
["5.16","Very High",8532]
["5.17","Very High",8533]
["5.18","High",8534]
["5.19","Medium",8535]
["5.2","Very High",8518]
["5.20","Medium",8536]
["5.21","Medium",8537]
["5.22","High",8539]
["5.23","Very High",8540]
["5.24","Very High",8541]
["5.25","Medium",8542]
["5.26","Medium",8543]
["5.27","Medium",8544]
["5.28","Very High",8545]
["5.29","High",8546]
["5.3","Low",8519]
["5.30","High",8547]
["5.31","High",8548]
["5.32","High",8549]
["5.33","High",8550]
["5.34","Low",8551]
["5.35","Medium",8552]
["5.36","Low",8553]
["5.37","Low",8554]
["5.38","High",8555]
["5.39","Very High",8556]
["5.4","High",8520]
["5.40","Very High",8557]
["5.41","Very High",8558]
["5.42","Medium",8559]
["5.43","High",8560]
["5.44","High",8561]
["5.45","Medium",8564]
["5.46","Medium",8565]
["5.47","Medium",8566]
["5.48","Medium",8567]
["5.5","Low",8521]
["5.6","Low",8522]
["5.7","Medium",8523]
["5.8","Medium",8524]
["5.9","Very High",8525]
["5.99","High",8568]
["6.1","Medium",8348]
["6.10","Low",8357]
["6.11","High",8358]
["6.12","Medium",8359]
["6.13","Low",8360]
["6.14","High",8361]
["6.15","High",8362]
["6.16","Very High",8363]
["6.17","Very High",8364]
["6.18","Medium",8365]
["6.19","Low",8366]
["6.2","High",8349]
["6.20","Medium",8367]
["6.21","High",8368]
["6.22","Medium",8369]
["6.3","Low",8350]
["6.4","High",8351]
["6.5","Medium",8352]
["6.6","Medium",8353]
["6.7","High",8354]
["6.8","High",8355]
["6.9","Low",8356]
["6.99","High",8370]
["7.1","High",8371]
["7.10","High",8380]
["7.11","High",8381]
["7.12","High",8382]
["7.13","Medium",8383]
["7.14","Medium",8384]
["7.15","High",8385]
["7.16","High",8386]
["7.17","High",8387]
["7.2","High",8372]
["7.3","Low",8373]
["7.4","Low",8374]
["7.5","Low",8375]
["7.6","Medium",8376]
["7.7","Low",8377]
["7.8","High",8378]
["7.9","High",8379]
["7.99","High",8388]
["8.1","Very High",8569]
["8.10","Very High",8578]
["8.100","Low",11227]
["8.101","Medium",11228]
["8.102","Low",11229]
["8.103","Low",11230]
["8.104","Low",11231]
["8.105","Medium",11232]
["8.106","Medium",11233]
["8.107","Low",11234]
["8.108","High",11235]
["8.109","Very High",11236]
["8.11","Medium",8579]
["8.110","High",11237]
["8.111","Medium",11238]
["8.112","High",11239]
["8.113","Medium",11240]
["8.114","Low",11241]
["8.115","High",11242]
["8.116","Medium",11243]
["8.117","Medium",11244]
["8.118","Medium",11245]
["8.119","High",11246]
["8.12","Medium",8580]
["8.120","High",11247]
["8.121","Medium",11248]
["8.122","High",11249]
["8.123","High",11250]
["8.124","Low",11251]
["8.125","High",11252]
["8.126","Medium",11253]
["8.127","Medium",11254]
["8.13","Medium",8581]
["8.14","Very High",8582]
["8.15","High",8583]
["8.16","Very High",8584]
["8.17","Low",8585]
["8.18","High",8586]
["8.19","High",8587]
["8.199","High",11255]
["8.2","Medium",8570]
["8.20","Medium",8588]
["8.21","High",8589]
["8.22","Very High",8590]
["8.23","Medium",8591]
["8.24","Medium",8592]
["8.25","Very High",8593]
["8.26","High",8594]
["8.27","Medium",8595]
["8.28","Medium",8596]
["8.29","High",8598]
["8.3","Very High",8571]
["8.30","High",8599]
["8.31","High",8600]
["8.32","Low",8601]
["8.33","Medium",8602]
["8.34","High",8603]
["8.35","Medium",8604]
["8.36","Medium",8605]
["8.37","High",8607]
["8.38","Medium",8608]
["8.39","Medium",8609]
["8.4","Medium",8572]
["8.40","High",8610]
["8.41","Medium",8611]
["8.42","Medium",8612]
["8.43","Very High",8613]
["8.44","High",8615]
["8.45","High",8616]
["8.46","Very High",8617]
["8.47","Very High",8618]
["8.48","Medium",8619]
["8.49","High",8620]
["8.5","Very High",8573]
["8.50","Medium",8621]
["8.51","Low",8622]
["8.52","Low",8623]
["8.53","Low",8624]
["8.54","High",8625]
["8.55","Low",11182]
["8.56","Medium",11183]
["8.57","Medium",11184]
["8.58","High",11185]
["8.59","High",11186]
["8.6","Medium",8574]
["8.60","High",11187]
["8.61","Medium",11188]
["8.62","Very High",11189]
["8.63","High",11190]
["8.64","Medium",11191]
["8.65","Low",11192]
["8.66","High",11193]
["8.67","High",11194]
["8.68","High",11195]
["8.69","Medium",11196]
["8.7","High",8575]
["8.70","Medium",11197]
["8.71","Very High",11198]
["8.72","Medium",11199]
["8.73","Medium",11200]
["8.74","High",11201]
["8.75","Medium",11202]
["8.76","Medium",11203]
["8.77","Medium",11204]
["8.78","Medium",11205]
["8.79","Medium",11206]
["8.8","Medium",8576]
["8.80","Medium",11207]
["8.81","Low",11208]
["8.82","Medium",11209]
["8.83","Low",11210]
["8.84","Low",11211]
["8.85","Medium",11212]
["8.86","Medium",11213]
["8.87","Medium",11214]
["8.88","Low",11215]
["8.89","High",11216]
["8.9","High",8577]
["8.90","High",11217]
["8.91","High",11218]
["8.92","Medium",11219]
["8.93","Low",11220]
["8.94","Low",11221]
["8.95","Medium",11222]
["8.96","Medium",11223]
["8.97","Low",11224]
["8.98","High",11225]
["8.99","Medium",11226]
["9.1","Low",8390]
["9.10","Medium",8399]
["9.11","Medium",8400]
["9.12","Medium",8401]
["9.13","Low",8402]
["9.14","Medium",8403]
["9.15","Medium",8404]
["9.16","High",8405]
["9.17","High",8406]
["9.18","Low",8407]
["9.19","Low",8408]
["9.2","Very High",8391]
["9.20","Medium",8409]
["9.21","Medium",8410]
["9.22","Low",8411]
["9.23","Low",8412]
["9.24","Medium",8413]
["9.25","Low",8414]
["9.26","Low",8415]
["9.27","Low",8416]
["9.28","Medium",8417]
["9.29","Low",8418]
["9.3","Very High",8392]
["9.4","High",8393]
["9.5","High",8394]
["9.6","Low",8395]
["9.7","Medium",8396]
["9.8","Medium",8397]
["9.9","Medium",8398]
["9.99","High",8419]

{"sheet":"Equipment_list","index":7,"n_rows":28,"n_cols":3,"rows_kept":28,"cut":false,"hidden":true,"merged":[]}
["TITLE","Equipment_list_description","ID"]
["Accommodation",null,12]
["Cargo Mach.",null,13]
["Critical Equip.",null,16]
["Deck - Machinery",null,18]
["Deck - Mooring Machinery",null,15]
["Deck - Pipe / Fittings",null,20]
["Documentation",null,21]
["E/R - Air Comp.",null,8]
["E/R - Aux. Engine",null,4]
["E/R - Aux. Mach.",null,7]
["E/R - Boiler",null,5]
["E/R - Main Engine",null,3]
["E/R - Pipes/ valves & fittings",null,9]
["E/R - Pumps",null,32]
["E/R - Purifier",null,6]
["Elect. Mach. & Equip.",null,10]
["Hull & Tanks",null,19]
["Inert Gas",null,14]
["LSA / FFA",null,17]
["Miscellaneous",null,22]
["Navigation - DGPS / EPFS / AIS",null,28]
["Navigation - ECDIS",null,25]
["Navigation - Echo Sounder / Speed Log",null,26]
["Navigation - GMDSS & Communication",null,23]
["Navigation - Others",null,11]
["Navigation - RADAR",null,24]
["Navigation - VDR / BNWAS",null,30]

{"sheet":"PSC_MOU","index":8,"n_rows":11,"n_cols":3,"rows_kept":11,"cut":false,"hidden":true,"merged":[]}
["TITLE","PSC_MOU_description","ID"]
["Asia and the Pacific",null,2]
["Caribbean",null,4]
["Europe and the North Atlantic",null,1]
["Latin America",null,3]
["The Black Sea region",null,6]
["The Indian Ocean",null,8]
["The Mediterranean",null,7]
["The Riyadh MoU",null,9]
["USCG",null,10]
["West and Central Africa",null,5]

{"sheet":"Inspection_type","index":9,"n_rows":13,"n_cols":2,"rows_kept":13,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Bunkering Audit",14]
["Cargo Audit",17]
["Engineering Audit",16]
["ISM Audit",2]
["ISPS Audit",3]
["IT Audit",10]
["MLC Audit",1]
["Mooring Audit",9]
["Nav Audit / Verification",8]
["Onboard Training",18]
["Ship Staff Insp.",15]
["Suptd. Insp.",13]

{"sheet":"Deficiency_Cause","index":10,"n_rows":8,"n_cols":3,"rows_kept":8,"cut":false,"hidden":true,"merged":[]}
["TITLE","Deficiency_Cause_description","ID"]
["Behaviour Based",null,1]
["Equipment Related",null,4]
["External Factors",null,5]
["Human Error",null,7]
["Inappropriate Procedure",null,8]
["Industry Issue",null,6]
["Knowledge Based",null,3]

{"sheet":"Observer_code","index":11,"n_rows":3,"n_cols":3,"rows_kept":3,"cut":false,"hidden":true,"merged":[]}
["TITLE","Observer_code_description","ID"]
["Owner / Marine / Tech. Suptd.",null,3]
["Ship Staff",null,2]

{"sheet":"Status_code","index":12,"n_rows":6,"n_cols":3,"rows_kept":6,"cut":false,"hidden":true,"merged":[]}
["TITLE","Status_code_description","ID"]
["Completed",null,6]
["Deferred to D D",null,5]
["In progress",null,3]
["Not Started",null,2]
["Waiting spare",null,4]

{"sheet":"PSC_ref_no","index":13,"n_rows":19,"n_cols":2,"rows_kept":19,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Alarms",9]
["Cargo operations including equipment",7]
["Certificates & Documentation",2]
["Dangerous Goods",13]
["Emergency Systems",5]
["Fire safety",8]
["ISM",16]
["ISPS",17]
["Life saving appliances",12]
["MLC, 2006",18]
["Other",19]
["Pollution Prevention",15]
["Propulsion and auxiliary machinery",14]
["Radio communication",6]
["Safety of Navigation",11]
["Structural condition",3]
["Water/Weathertight condition",4]
["Working and Living Conditions",10]

{"sheet":"Risk_value_of_obs","index":14,"n_rows":1,"n_cols":2,"rows_kept":1,"cut":false,"hidden":true,"merged":[]}
["Risk Value of observation","ID"]

{"sheet":"Year","index":15,"n_rows":18,"n_cols":1,"rows_kept":18,"cut":false,"hidden":true,"merged":[]}
["Year"]
[2014]
[2015]
[2016]
[2017]
[2018]
[2019]
[2020]
[2021]
[2022]
[2023]
[2024]
[2025]
[2026]
[2027]
[2028]
[2029]
[2030]

{"sheet":"Month","index":16,"n_rows":13,"n_cols":1,"rows_kept":13,"cut":false,"hidden":true,"merged":[]}
["Month"]
["Jan"]
["Feb"]
["Mar"]
["Apr"]
["May"]
["Jun"]
["Jul"]
["Aug"]
["Sep"]
["Oct"]
["Nov"]
["Dec"]

{"sheet":"Date_","index":17,"n_rows":32,"n_cols":1,"rows_kept":32,"cut":false,"hidden":true,"merged":[]}
["Date"]
["01"]
["02"]
["03"]
["04"]
["05"]
["06"]
["07"]
["08"]
["09"]
[10]
[11]
[12]
[13]
[14]
[15]
[16]
[17]
[18]
[19]
[20]
[21]
[22]
[23]
[24]
[25]
[26]
[27]
[28]
[29]
[30]
[31]

{"sheet":"Sheet1","index":18,"n_rows":24,"n_cols":6,"rows_kept":24,"cut":false,"hidden":true,"merged":[]}
[]
[null,"ID","E",null,"Date Recorded",1]
[null,"UNIQUE ID","F",null,"Type of Deficiency",2]
[1,"Date Recorded","G",null,"Observer code",3]
["ignore","Vessel Type","H",null,"Type of Inspection",4]
[null,"Internal / External","I",null,"Description of Deficiency",5]
[null,"Drydock","J",null,"Equipment Categories",6]
[null,"Information Sharing","K",null,"Area of Observation",7]
[null,"Critical_item","L",null,"Deficiency Cause",8]
[null,"Deficiency Type","M",null,"VIQ Ref Number",9]
[null,"Deficiency Cause","N",null,"Risk Value of Obs",10]
[null,"Inspection Type","O",null,"PSC Ref Number",11]
[null,"Equipments","P",null,"PSC MOU ID",12]
[null,"VIQ Reference Number","Q",null,"Action Taken or Required",13]
[null,"Risk Value of the observation","R",null,"Target Date",14]
[null,"PSC Reference Number","S",null,"PO Ref No.",15]
[null,"PSC MOU","T",null,"Status Code",16]
[null,"Observer Code","U",null,"Date Completed",17]
[null,"Target Date","V",null,"Drydock",18]
[null,"Status Code","W",null,"Info Sharing",19]
[null,"Description of Deficiency","X",null,"Critical Item Flag",20]
[null,"Action taken / required","Y",null,"Audit Type",21]
[null,"PO ref no","Z"]
[null,"Date completed","AA"]

{"sheet":"Ship_information","index":19,"n_rows":2,"n_cols":3,"rows_kept":2,"cut":false,"hidden":true,"merged":[]}
["Ship_ID","Ship_Name","FILE_NAME"]
["36","ZENO (16-03-2021)","36_1615892699581.xlsm"]

{"sheet":"External_Deficiency_type","index":20,"n_rows":5,"n_cols":3,"rows_kept":5,"cut":false,"hidden":true,"merged":[]}
["TITLE","Type of deficiency_description","ID"]
["Condn of Class / Memo",null,5]
["Defect",null,1]
["Non Conformity",null,2]
["Observation",null,3]

{"sheet":"External_Inspection_type","index":21,"n_rows":11,"n_cols":2,"rows_kept":11,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Cargo Audit",17]
["Flag State Insp.",5]
["ISM Audit",2]
["ISPS Audit",3]
["MLC Audit",1]
["Nav Audit / Verification",8]
["OM Insp. (Eg. SIRE / CDI etc.)",6]
["Others (Eg. Insurance etc.)",12]
["PSC Inspection",4]
["Terminal Insp.",11]

{"sheet":"External_Observer_code","index":22,"n_rows":7,"n_cols":3,"rows_kept":7,"cut":false,"hidden":true,"merged":[]}
["TITLE","Observer_code_description","ID"]
["Class Surveyor",null,4]
["FSC Inspector",null,5]
["Others (Eg. Insurance etc.)",null,9]
["PSC Insp.",null,6]
["SIRE / CDI Insp.",null,8]
["Terminal Insp.",null,7]

{"sheet":"Sheet Version","index":23,"n_rows":2,"n_cols":2,"rows_kept":2,"cut":false,"hidden":true,"merged":[]}
["Version","Title"]
["2.0","Version 2.0"]