{"text_format":"1","workbook":"xlsx","n_sheets":24,"sheets":["Mainsheet","Completed","Calc","Areaofobs","Vessel_type","Deficiency_type","VIQrefno","Equipment_list","PSC_MOU","Inspection_type","Deficiency_Cause","Observer_code","Status_code","PSC_ref_no","Risk_value_of_obs","Year","Month","Date_","Sheet1","Ship_information","External_Deficiency_type","External_Inspection_type","External_Observer_code","Sheet Version"],"not_rendered":{"charts":0,"images":5,"macros":1,"external_links":0,"defined_names":12,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Mainsheet","index":0,"n_rows":69,"n_cols":28,"rows_kept":69,"cut":false,"hidden":false,"merged":[[10,8,10,9],[10,12,10,13],[12,6,12,27],[8,6,8,27]]}
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,"Defect - Damage Monitoring Sheet"]
[]
[null,null,null,null,null,null,null,"Date of Report","16-Mar-2021",null,null,"Ship Name","GILOS (16-03-2021)"]
[]
[null,null,null,null,null,null,"VERSION : 2.0"]
[]
[]
[]
[null,null,null,null,"ID","UNIQUE ID","Date Recorded","Type of Deficiency","Observer code","Type of Inspection","Description of Deficiency","Equipment Categories","Area of Observation","Deficiency Cause","VIQ Ref Number","Risk Value of Obs","PSC Ref Number","PSC MOU ID","Action Taken or Required","Target Date","PO Ref No.","Status Code","Date Completed","Drydock","Info Sharing","Critical Item","Audit Type","Superintendent Remarks"]
[null,null,null,null,13806,"103_29/8/2020 6:01:56 AM","2020-08-20","Defect,Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","The air filter and lubricator unit for both the gangways found missing","Deck - Pipe / Fittings","Safety / LSA / FFA","Equipment Related",5.47,"Medium","Not Applicable","Not Applicable","Awaiting spares.","2021-02-28",null,"In progress",null,"No","No","No","Internal","Same is ordered ,"]
[null,null,null,null,13817,"103_29/8/2020 6:06:29 AM","2020-08-21","Observation","Ship Staff","Ship Staff Insp.","Many COW machines for the cargo tanks found not working with the working pressure and needs to be turned manually","Cargo Mach.","Cargo / Ballast Systems","Equipment Related",8.34,"High","Not Applicable","Not Applicable","Spares recevied on 22 Apr 2021. Overhauling in progress.","2021-02-28",null,"In progress",null,"No","No","No","Internal","Work Is in progress to be completed by 28-Dec-2021"]
[null,null,null,null,13790,"103_28/8/2020 6:01:25 AM","2020-12-20","Observation","Ship Staff","Ship Staff Insp.","Starbord provision crane found leaking from the RAM cylinder","Deck - Machinery","MARPOL Related","Equipment Related",8.6300000000000008,"High","Not Applicable","Not Applicable","RAM seal received in Fujairah on 03 April 2021. Seal to be renewed.","2021-03-20",null,"Waiting spare",null,"No","No","No","Internal"]
[null,null,null,null,13791,"103_28/8/2020 6:09:40 AM","2020-12-20","Observation","Ship Staff","Ship Staff Insp.","Port provision crane found leaking from the hose connection block on the cylinder RAM","Deck - Machinery","MARPOL Related","Equipment Related",8.6300000000000008,"High","Not Applicable","Not Applicable","New Block received. Leaking block to be renewed.","2021-03-20",null,"Waiting spare",null,"No","No","No","Internal"]
[null,null,null,null,17105,"103_Thu Jan 14 2021 07:47:24 GMT+0000","2020-12-27","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Stbd Gangway pneumatic lines are in poor condition.","Deck - Pipe / Fittings","General Appearance","Equipment Related",null,null,"Not Applicable","Not Applicable","Pipelines renewed. Awaiting Air filters and Lubricators.","2021-01-26",null,"In progress",null,"No","No","No","Internal"]
[null,null,null,null,17106,"103_Thu Jan 14 2021 08:07:42 GMT+0000","2020-12-27","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Railings of walkway on main deck have scattered thick rust spots.","Deck - Pipe / Fittings","General Appearance","External Factors","12.9","High","","","Derusting and painting of railings of safety walkway in progress. ","2021-03-26","","In progress",null,"No","No","No","Internal"]
[null,null,null,null,17107,"103_Thu Jan 14 2021 08:09:40 GMT+0000","2020-12-27","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Provision cranes’ jibs is rusty.","Deck - Machinery","Cargo / Ballast Systems","Equipment Related","8.73","Medium","","","Port side Provision crane derusting completed. Stbd side Provision crane in progress.","2021-03-26","","In progress",null,"No","No","No","Internal"]
[null,null,null,null,17119,"103_Thu Jan 14 2021 10:10:10 GMT+0000","2020-12-27","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Auxiliary boiler FO pump no.1 leaking from mechanical seal.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related",null,null,"Not Applicable","Not Applicable","Auxiliary boiler FO pump no.1 leaking from mechanical seal. Same needs to be rectified.","2021-01-26","GILO210018","Waiting spare",null,"No","No","No","Internal"]
[null,null,null,null,null,"103_7/4/2021 8:08:24 AM","2021-03-01","Defect","Ship Staff","Ship Staff Insp.","Main LO pump no.1 motor controller operating erratically.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related",10.37,"Medium","Not Applicable","Not Applicable","Need to replace the motor controller for NO.1 Main LO pump","2021-07-01","GILO210062","Waiting spare",null,"No",null,null,"Internal"]
[null,null,null,null,null,"103_26/3/2021 7:23:20 PM","2021-03-26","Defect","Ship Staff","Ship Staff Insp.","Mooring Winch brake band hinges thinned down","Deck - Mooring Machinery","Mooring","Equipment Related",9.15,"Medium","Not Applicable","Not Applicable","Wasted sections to be cropped and new inserts to be welded in place. 6 Hinges repaired. Others in progress.","2021-05-31",null,"In progress",null,"No",null,null,"Internal"]
[null,null,null,null,null,"103_26/3/2021 7:25:56 PM","2021-03-26","Defect","Ship Staff","Ship Staff Insp.","Mooring winch isolation valves are heavily rusted. Valve handles also rusted and wasted.\t","Deck - Mooring Machinery","Mooring","Equipment Related",9.1999999999999993,"Very High","Not Applicable","Not Applicable","Most of the valves derusted and painted. Few more valves remaining. Only 2 Valves remaining.","2021-05-31",null,"In progress",null,"No",null,null,"Internal"]
[null,null,null,null,null,"103_26/3/2021 7:29:14 PM","2021-03-26","Defect","Ship Staff","Ship Staff Insp.","Two crew members having defective Vaccum Toilet system. They have to open the toilet inspection port and manually push the control valve to operate the Vaccum toilet system.","Accommodation","General Appearance","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","New discharge valve's need to be fitted. PO raised for the same. Awaiting spares.","2021-05-31","GILO210026","Waiting spare",null,"No",null,null,"Internal"]
[null,null,null,null,null,"103_26/3/2021 7:38:28 PM","2021-03-26","Defect","Ship Staff","Ship Staff Insp.","Lot of Pipes and Pipe supports on Deck are wasted.\t","Deck - Pipe / Fittings","General Appearance","Equipment Related",11.4,"Very High","Not Applicable","Not Applicable","Wasted Pipes & pipe supports to be renewed. This job can be be carried out only when vessel is gas free.","2021-09-26",null,"Not Started",null,"No",null,null,"Internal"]
[null,null,null,null,null,"103_26/3/2021 7:43:30 PM","2021-03-26","Defect","Ship Staff","Ship Staff Insp.","Port side hose handling crane runner wire operating lever very hard to operate and does not return back to orginal posn by itself.","Deck - Machinery","Cargo / Ballast Systems","Equipment Related",8.5,null,"Not Applicable","Not Applicable","Control valve to be overhauled.","2021-04-30",null,"Not Started",null,"No",null,null,"Internal"]
[null,null,null,null,null,"103_26/3/2021 7:53:21 PM","2021-03-26","Defect","Ship Staff","Ship Staff Insp.","Navtex Receiver not receiving 518 Khz messages.","Navigation - GMDSS & Communication","Navigation","Equipment Related",4.7,"High","Not Applicable","Not Applicable","Suspect Navtex Receiver faulty. Awaiting office instructions.","2021-04-30",null,"In progress",null,"No",null,null,"Internal"]
[null,null,null,null,null,"103_26/3/2021 7:59:02 PM","2021-03-26","Defect","Ship Staff","Ship Staff Insp.","Minor leak from Steam Ballast Pump casing top seal.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related",8.19,"High","Not Applicable","Not Applicable","Ballast Pump seal to be overhauled and renewed if required.","2021-04-30",null,"Not Started",null,"No",null,null,"Internal"]
[null,null,null,null,null,"103_26/3/2021 8:01:00 PM","2021-03-26","Defect","Ship Staff","Ship Staff Insp.","Back up Oxygen Sensor not working.\t","Inert Gas","Cargo / Ballast Systems","Equipment Related",8.2200000000000006,"Very High","Not Applicable","Not Applicable","New Oxygen Sensor spare is required. ","2021-07-30",null,"In progress",null,"No",null,null,"Internal"]
[null,null,null,null,null,"103_26/3/2021 8:02:51 PM","2021-03-26","Defect","Ship Staff","Ship Staff Insp.","Remote RPM control of No 1 Ballast Pump not operational. Unable to control ballast pump from CCR\t","Cargo Mach.","Cargo / Ballast Systems","Equipment Related",8.19,"High","Not Applicable","Not Applicable","Speed control switch needs to be renewed.","2021-04-30","GILO210086","Waiting spare",null,"No",null,null,"Internal"]
[null,null,null,null,null,"103_26/3/2021 8:08:17 PM","2021-03-26","Defect","Ship Staff","Ship Staff Insp.","Most of the PV Valves are leaking\t","Inert Gas","Cargo / Ballast Systems","Equipment Related",8.41,"Medium","Not Applicable","Not Applicable","RO raised for spare seats and disks.","2021-04-30",null,"Waiting spare",null,"No",null,null,"Internal"]
[null,null,null,null,null,"103_26/3/2021 8:17:09 PM","2021-03-26","Defect","Ship Staff","Ship Staff Insp.","No 2 Cargo eductor gauges in the CCR Panel  are erractic","Cargo Mach.","Cargo / Ballast Systems","Equipment Related",8.1199999999999992,"Medium","Not Applicable","Not Applicable","Pressure transmitters found defective. RO to be raised for new pressure transmitter.","2021-07-30",null,"Waiting spare",null,"No",null,null,"Internal"]
[null,null,null,null,null,"103_26/3/2021 8:19:10 PM","2021-03-26","Defect","Ship Staff","Ship Staff Insp.","Cargo & Ballast Pump Vibration Monitor system giving alarm when cargo & ballast pumps are running.\t","Cargo Mach.","Cargo / Ballast Systems","Equipment Related",8.1199999999999992,"Medium","Not Applicable","Not Applicable","Vibration Monitoring system was checked and vibration sensors tightness were checked. Found tight. The distance of the sensor from the shaft was also found ok. Need further investigation during running of pump.","2021-07-30",null,"In progress",null,"No",null,null,"Internal"]
[null,null,null,null,null,"103_26/3/2021 8:23:01 PM","2021-03-26","Defect","Ship Staff","Ship Staff Insp.","COW & Hydrualic pipe lines on deck are heavily rusted.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related",11.4,"Very High","Not Applicable","Not Applicable","Derusting and painting in progress.","2021-05-31",null,"In progress",null,"No",null,null,"Internal"]
[null,null,null,null,null,"103_26/3/2021 8:27:39 PM","2021-03-26","Defect","Ship Staff","Ship Staff Insp.","COW Pipeline valves - Handles, valve locking grooves and valve indicators are wasted.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related",8.34,"High","Not Applicable","Not Applicable","RO raised for Handles, valve locking grooves and valve indicators.","2021-04-30",null,"Waiting spare",null,"No",null,null,"Internal"]
[null,null,null,null,null,"103_26/3/2021 8:29:08 PM","2021-03-26","Defect","Ship Staff","Ship Staff Insp.","No 3C COT - Vapour lock cap missing\t","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related",8.1199999999999992,null,"Not Applicable","Not Applicable","Ro raised for spare vapour lock cap","2021-04-30",null,"Waiting spare",null,"No",null,null,"Internal"]
[null,null,null,null,null,"103_26/3/2021 8:32:59 PM","2021-03-26","Defect","Ship Staff","Ship Staff Insp.","One of the UTI onboard leaking Inert gas when used on deck.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related",8.1199999999999992,"Medium","Not Applicable","Not Applicable","This is a Rtex type UTI ( Restricted type) which will leak inert gas when used. Hence requesting for Gtex ( Gas Tight) model UTI.","2021-07-31",null,"Not Started",null,"No",null,null,"Internal"]
[null,null,null,null,null,"103_26/3/2021 8:38:24 PM","2021-03-26","Defect","Ship Staff","Ship Staff Insp.","Main IG Pipe line on deck having a soft patch near to the Drain pipe\t","Inert Gas","Cargo / Ballast Systems","Equipment Related",8.3000000000000007,"High","Not Applicable","Not Applicable","Pipe to be dismantled and repaired.","2021-09-30",null,"Not Started",null,"No",null,null,"Internal"]
[null,null,null,null,null,"103_26/3/2021 8:43:13 PM","2021-03-26","Defect","Ship Staff","Ship Staff Insp.","No 1 Ballast Pump sucton pipe line having soft patch","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related",8.19,"High","Not Applicable","Not Applicable","Permanent repairs to be carried out.","2021-09-30",null,"Not Started",null,"No",null,null,"Internal"]
[null,null,null,null,null,"103_26/3/2021 8:46:02 PM","2021-03-26","Defect","Ship Staff","Ship Staff Insp.","Ballast Overboard valve remote opening hydraulic actuator supports wasted","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related",8.19,null,"Not Applicable","Not Applicable","Wasted supports to be renewed. This can be carried out only when the ship is gas free.","2021-09-30",null,"Not Started",null,"No",null,null,"Internal"]
[null,null,null,null,null,"103_26/3/2021 8:47:48 PM","2021-03-26","Defect","Ship Staff","Ship Staff Insp.","Only one Gangway Air Motor is operational. Other 3 Air Motors are not operational.","Deck - Machinery","General Appearance","Equipment Related",5.47,"Medium","Not Applicable","Not Applicable","New Air Motor received at Fujairah on 03 April 2021.But air filters and air lubricators NOT received.","2021-05-31",null,"Waiting spare",null,"No",null,null,"Internal"]
[null,null,null,null,null,"103_26/3/2021 8:51:25 PM","2021-03-26","Defect","Ship Staff","Ship Staff Insp.","Air filters and Lubricators missing from Gangway Air Motor pipe lines","Deck - Pipe / Fittings","General Appearance","Equipment Related",5.47,"Medium","Not Applicable","Not Applicable","Awaiting spares.","2021-07-30",null,"Waiting spare",null,"No",null,null,"Internal"]
[null,null,null,null,null,"103_26/3/2021 9:03:51 PM","2021-03-26","Defect","Ship Staff","Ship Staff Insp.","Lot of Cable conduit pipes in Accommodation not sealed/closed after passing cables.","Accommodation","General Appearance","Equipment Related",11.4,"Very High","Not Applicable","Not Applicable","Open cable conduit pipes to be sealed with appropriate sealing material.","2021-04-30",null,"Not Started",null,"No",null,null,"Internal"]
[null,null,null,null,null,"103_26/3/2021 9:09:04 PM","2021-03-26","Defect","Ship Staff","Ship Staff Insp.","Transmitting Magnetic Compass (TMC) not connected to OCA/HDM Alarm unit. TMC unit and OCA/HDM Units are not compatible. TMC is a new Unit. OCA/HDM Unit was installed when vessel was constructed.","Navigation - Others","Navigation","Equipment Related",4.7,"High","Not Applicable","Not Applicable","Awaiting office instructions. ","2021-05-31",null,"Not Started",null,"No",null,null,"Internal"]
[null,null,null,null,null,"103_26/3/2021 9:10:35 PM","2021-03-26","Defect","Ship Staff","Ship Staff Insp.","Stripping Pump leaking from seal.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related",8.8000000000000007,null,"Not Applicable","Not Applicable","One seal renewed. Other seal to be renewed.","2021-04-30",null,"In progress",null,"No",null,null,"Internal"]
[null,null,null,null,null,"103_26/3/2021 9:12:12 PM","2021-03-26","Defect","Ship Staff","Ship Staff Insp.","Cargo Pump AUS System GEV valves near pumproom entrance - Valve indicator cover missing.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related",8.8000000000000007,"Medium","Not Applicable","Not Applicable","RO to be raised for new cover.","2021-07-31",null,"Waiting spare",null,"No",null,null,"Internal"]
[null,null,null,null,null,"103_26/3/2021 9:16:03 PM","2021-03-26","Defect","Ship Staff","Ship Staff Insp.","Shower Mixers are bypassing and Hot water coming in cold water lines in accommodation.","Accommodation","General Appearance","Equipment Related",11.13,"Low","Not Applicable","Not Applicable","RO raised for new Shower mixers.","2021-05-31",null,"Waiting spare",null,"No",null,null,"Internal"]
[null,null,null,null,null,"103_26/3/2021 9:20:57 PM","2021-03-26","Defect","Ship Staff","Ship Staff Insp.","Only a copy of Suez Canal Tonnage certificate available onboard. Orginal missing.\t","Documentation","Cert. & Docu.","Equipment Related",2.1,null,"Not Applicable","Not Applicable","Applied to class for reissuing new Suez Canal Tonnage Certificate.","2021-04-30",null,"In progress",null,"No",null,null,"Internal"]
[null,null,null,null,null,"103_26/3/2021 9:23:22 PM","2021-03-26","Defect","Ship Staff","Ship Staff Insp.","All the Rudder Angle indicators are displaying erractic values +/- 1 Deg.","Navigation - Others","Navigation","Equipment Related",4.7,"High","Not Applicable","Not Applicable","Carried out checks as per office instructions during the vessel's call at Fujariah anchorage. During the port movement the indicators are displaying correct reading but during starboard movement there is an error of about 1 deg.","2021-07-15",null,"In progress",null,"No",null,null,"Internal"]
[null,null,null,null,null,"103_26/3/2021 9:25:42 PM","2021-03-26","Defect","Ship Staff","Ship Staff Insp.","Autopilot Control Panel lights faded, unable to see the text in the panel during day time.","Navigation - Others","Navigation","Equipment Related",4.7,"High","Not Applicable","Not Applicable","Awaiting Office instructions.","2021-04-30",null,"Not Started",null,"No",null,null,"Internal"]
[null,null,null,null,null,"103_26/3/2021 9:28:52 PM","2021-03-26","Defect","Ship Staff","Ship Staff Insp.","Rate of Turn Indicator night backlight is very dim. Very difficult to see at night.","Navigation - Others","Navigation","Equipment Related",4.7,"High","Not Applicable","Not Applicable","Bulb to be renewed. No spare bulb found on board.","2021-07-30",null,"Not Started",null,"No",null,null,"Internal"]
[null,null,null,null,null,"103_2/4/2021 12:37:04 AM","2021-03-26","Defect","Ship Staff","Ship Staff Insp.","Few sounding pipes for ballast tanks chocked.\t","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related",2.16,"Medium","Not Applicable","Not Applicable","Chocked sounding pipes to be cleared.","2021-07-31",null,"In progress",null,"No",null,null,"Internal"]
[null,null,null,null,null,"103_1/4/2021 11:50:40 AM","2021-03-27","Defect","Ship Staff","Ship Staff Insp.","Bridge watch unit is showing a power failure alarm\t","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related",10.4,"High","Not Applicable","Not Applicable","Vessel doesnot have a 120 ohm resistor. Same has been asked from office. Awaiting spare.","2021-08-01",null,"Waiting spare",null,"No",null,null,"Internal"]
[null,null,null,null,null,"103_2/4/2021 8:34:56 AM","2021-03-28","Defect","Ship Staff","Ship Staff Insp.","Engine room water cooler not operational\t","Accommodation,Miscellaneous","MLC Related","Equipment Related",11.13,"Low","Not Applicable","Not Applicable","Need to fabricate a pipeline and for water inlet","2021-06-01",null,"Not Started",null,"No",null,null,"Internal"]
[null,null,null,null,null,"103_7/4/2021 7:57:20 AM","2021-03-29","Observation","Ship Staff","Ship Staff Insp.","LT cooler no.1 sea water outlet valve not holding","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","The valve needs to be renewed","2021-07-01","GILO210091","Waiting spare",null,"No",null,null,"Internal"]
[null,null,null,null,null,"103_12/4/2021 2:49:11 PM","2021-04-12","Defect","Ship Staff","Ship Staff Insp.","1 Mooring wire found with more than 10% broken strands in the eye.","Deck - Mooring Machinery","Mooring","Equipment Related",9.17,"High","Not Applicable","Not Applicable","Wire to be replaced with new wire. RO raised.","2021-05-31",null,"Waiting spare",null,"No",null,null,"Internal"]
[null,null,null,null,null,"103_12/4/2021 2:58:01 PM","2021-04-12","Defect","Ship Staff","Ship Staff Insp.","Stbd side Provision crane wire heaving/lowering winch leaking oil.","Deck - Machinery","General Appearance","Equipment Related",8.6300000000000008,"High","Not Applicable","Not Applicable","RO to be raised for leaking control block.","2021-07-31",null,"Waiting spare",null,"No",null,null,"Internal"]
[null,null,null,null,null,"103_12/4/2021 3:03:41 PM","2021-04-12","Defect","Ship Staff","Ship Staff Insp.","Stbd Side Life Boat skates and davit chockes are brittle and cracking.","LSA / FFA","Safety / LSA / FFA","Equipment Related",5.28,"Very High","Not Applicable","Not Applicable","RO riased for new skates and chockes.","2021-04-30",null,"Waiting spare",null,"No",null,null,"Internal"]
[null,null,null,null,null,"103_12/4/2021 3:05:36 PM","2021-04-12","Defect","Ship Staff","Ship Staff Insp.","Few rollers in the ship side for Pilot ladder lowering found wasted and holed.\t","Deck - Mooring Machinery","Mooring","Equipment Related",9.18,"Low","Not Applicable","Not Applicable","Wasted section to be cropped and new inserts to be put in place.","2021-05-31",null,"Not Started",null,"No",null,null,"Internal"]
[null,null,null,null,null,"103_1/5/2021 2:43:47 PM","2021-04-27","Defect","Ship Staff","Ship Staff Insp.","Main HFO flowmeter showing erratic readings.\t","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Vanes and push rods have already been renewed. Bearings have also been renewed. Still the problem persists. Awaiting further instructions from the makers.","2021-07-01",null,"In progress",null,"No",null,null,"Internal"]
[null,null,null,null,null,"103_2/5/2021 8:40:15 PM","2021-05-02","Defect","Ship Staff","Ship Staff Insp.","Few Accommodation B Class fire doors found missing with locks, leaving a opening in the doors.","Accommodation","Safety / LSA / FFA","Equipment Related",5.0999999999999996,"High","Not Applicable","Not Applicable","RO raised for locks.","2021-07-01",null,"Waiting spare",null,"No",null,null,"Internal"]
[null,null,null,null,null,"103_2/5/2021 8:45:16 PM","2021-05-02","Defect","Ship Staff","Ship Staff Insp.","Anchor Hawse Pipe covers hinges are damaged\t\t","Deck - Pipe / Fittings","Mooring","Equipment Related",7.12,"High","Not Applicable","Not Applicable","New hinges to be faricated and fitted with nut bolts.","2021-07-31",null,"Not Started",null,"No",null,null,"Internal"]
[null,null,null,null,null,"103_25/5/2021 9:09:39 AM","2021-05-22","Defect","Ship Staff","Ship Staff Insp.","Incinerator sluice door not operating.\t","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Need to renew a solenoid valve. Vessel does not have spare on board. Need to raise PO for the same. Currently trying to overhaul the solenoid valve with old used spares.","2021-08-01",null,"In progress",null,"No",null,null,"Internal"]
[null,null,null,null,null,"103_26/6/2021 7:45:17 AM","2021-06-07","Observation","Ship Staff","Ship Staff Insp.","Starboard hose handling leak has a minor oil leak from winch load control valve connector and hose.","Deck - Machinery","Cargo / Ballast Systems","Equipment Related",8.5,"Very High","Not Applicable","Not Applicable","Need to replace the control block and leaky hose.","2021-08-01",null,"Not Started",null,"No",null,null,"Internal"]

{"sheet":"Completed","index":1,"n_rows":308,"n_cols":28,"rows_kept":308,"cut":false,"hidden":false,"merged":[[10,8,10,9],[10,12,10,13],[12,6,12,27],[8,6,8,27]]}
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,"Defect - Damage Monitoring Sheet"]
[]
[null,null,null,null,null,null,null,"Date of Report","16-Mar-2021",null,null,"Ship Name","GILOS (16-03-2021)"]
[]
[null,null,null,null,null,null,"VERSION : 2.0"]
[]
[]
[]
[null,null,null,null,"ID","UNIQUE ID","Date Recorded","Type of Deficiency","Observer code","Type of Inspection","Description of Deficiency","Equipment Categories","Area of Observation","Deficiency Cause","VIQ Ref Number","Risk Value of Obs","PSC Ref Number","PSC MOU ID","Action Taken or Required","Target Date","PO Ref No.","Status Code","Date Completed","Drydock","Info Sharing","Critical Item","Audit Type","Superintendent Remarks"]
[null,null,null,null,10895,"103_29/3/2020 5:20:34 PM","2020-03-19","Defect,Observation","Ship Staff","Ship Staff Insp.","Discharge pipeline for No.2 WBP found holed\t","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","","","","","The pipeline section removed and hotwork carried out. Pipleline fitted in place and tested. Found satisfactory","2020-05-30","","Completed","2020-04-04","No","No","No","Internal"]
[null,null,null,null,10897,"103_29/3/2020 5:25:46 PM","2020-03-19","Critical Equipment,Defect,Observation","Ship Staff","Ship Staff Insp.","The UTIs used for Cargo tanks gauging found damaged with soft patch put","Cargo Mach.,Hull & Tanks","Cargo / Ballast Systems","Behaviour Based,Equipment Related,Human Error","","","","","1 UTI already shore serviced and calibrated. As per office communication and instructions, Other UTI also is acceptable.","2020-05-30","","Completed","2020-07-06","No","No","No","Internal","Operation department will revert on same."]
[null,null,null,null,10898,"103_30/3/2020 7:56:09 PM","2020-03-19","Critical Equipment","Ship Staff","Ship Staff Insp.","Fire alarm panel System fault status. 12 Smoke detectors and 2 flame detectors not working and broken from base.","Critical Equip.","Emgcy. Systems","Equipment Related","5.4","High","","","Service engineer attended vessel and all detectors and MCP replaced with new received spare","2020-05-30","GILO205074,205075,205105","Completed","2020-08-20","No","No","No","Internal","08-June-2020:\nComplete  Fire  Alarm Panel will be modified by Martek Singapore. Mr. Kamlesh is working on same."]
[null,null,null,null,10899,"103_30/3/2020 8:03:06 PM","2020-03-19","Defect","Owner / Marine / Tech. Suptd.","Engineering Audit","Echo Sounder: Aft transducer working erratic. To be investigated and repair","Navigation - Echo Sounder / Speed Log","Navigation","Equipment Related","4.3","Medium","","","awaiting Shore service","2020-05-30","","Completed","2020-06-09","No","No","No","Internal","09-June-2020:\nBelow mentioned issue of Echo sounder has been attended and problem with the selector switch has been sorted out."]
[null,null,null,null,10900,"103_30/3/2020 8:15:04 PM","2020-03-19","Defect","Owner / Marine / Tech. Suptd.","Engineering Audit","VDR JCY-1000, Need to be upgraded. Maker cannot carry out APT Test due to fault and non-availability of spares","Navigation - VDR / BNWAS","Navigation","Equipment Related","5.3","Low","","","Hardware and cable layout job, completed","2020-03-30","","Completed","2020-08-17","No","No","No","Internal","New VDR arranged by Owners"]
[null,null,null,null,10901,"103_30/3/2020 8:24:03 PM","2020-03-19","Critical Equipment","Owner / Marine / Tech. Suptd.","Engineering Audit","Fire Fighting Walkie Talkies: There are only two dedicated walkies talkies onboard. Two more need to be supplied as there are four fire man outfits","LSA / FFA","Communication","External Factors","5.3","Low","","","Vessel recieved 2 new Radios for fire fighting. Existing radios landed ashore for frequency set. Same recieved and found matching with ship's radio frequency.","2020-05-30","GILO200004","Completed","2020-07-22","No","No","No","Internal","08-June-2020\nGILO200004 is approved for supply. This will be supplied by Goodwood."]
[null,null,null,null,10902,"103_30/3/2020 8:48:15 PM","2020-03-19","Observation","Owner / Marine / Tech. Suptd.","Engineering Audit","Wifi and crew internet PC installation.\n\nETO need to lay LAN cables from CCR to each smoke room and install wifi and crew internet PC","Miscellaneous","Communication","Equipment Related","","","","","Wifi installed.","2020-04-30","","Completed","2020-07-01","No","No","No","Internal","08-June-2020:\n\nIs this still open."]
[null,null,null,null,11468,"103_1/4/2020 3:19:19 AM","2020-03-19","Non Conformity","Owner / Marine / Tech. Suptd.","Ship Staff Insp.","Clear view screen not provided on Bridge","Navigation - Others","Navigation","Inappropriate Procedure","","","","","Informed office.","2020-04-15","","Completed","2020-06-09","No","No","No","Internal","Clear View Screen is not mandatory. Hence the defect is closed. \n\n//QTE//\n\nAll bridge front windows shall be provided with efficient cleaning, de-icing and de-misting devices. In case of a totally enclosed bridge also the aft facing windows and the side windows (except sliding windows) at the docking stations shall be provided with such devices.\n\nThe use of clear view screens (rotating windows) is not required. However, if fitted, they shall not be installed in windows in front of any workstation.\n\n//UNQTE//"]
[null,null,null,null,11529,"103_30-Apr-20 9:18:07 PM","2020-03-20","Observation","Ship Staff","Ship Staff Insp.","HEADING MONITOR/ OFFCOURSE ALARM UNIT LED DISPLAY NOT WORKING PROPERLY/ UNREADABLE","Navigation - Others","Navigation","Equipment Related","","","","","AS PER OWNER'S TECHNICIAN & SPARES TO BE SENT ON BOARD, SERVICE ENGINEER ATTENDED AT SINGAPORE ON 20-AUG-2020 AND CHANGED LCD SCREEN STILL ERROR IN MAGNETIC COMPASS HEADING EXISTS. AS PER TECHNICIAN SUGGEST PANEL TO BE REPLACED. Vessel found out that there is no connection provided from TMC to Heading monitor inside the steering stand. This is as per design by maker.","2020-05-10","","Completed","2020-11-15","No","No","No","Internal","07-June-2020:\nHas vessel raised any requisition for same."]
[null,null,null,null,10903,"103_30/3/2020 8:12:15 PM","2020-03-20","Defect","Owner / Marine / Tech. Suptd.","Nav Audit / Verification","ECDIS JRC, JAN-901B: Manual update not working and software to be upgraded","Navigation - ECDIS","Navigation","Equipment Related","5.1","Very High","","","shore service completed","2020-05-30","","Completed","2020-03-20","No","No","No","Internal"]
[null,null,null,null,10904,"103_30/3/2020 8:08:06 PM","2020-03-20","Defect","Owner / Marine / Tech. Suptd.","Engineering Audit","Many window wipers are not working. Routine maintenance to be carried out and order the relevant spares","Navigation - Others","Navigation","Equipment Related","5.1","Very High","","","WIPER ASSEMBLY DISMENATLED , DEFECTIVE PARTS REPLACED WITH SPARE , V-BELT, MOTOR ETC. ALL TRIED OUT WORKING SATISFACTORY","2020-05-30","GILOS - 036 - WINDOW WIPER","Completed","2020-07-02","No","No","No","Internal","Date: 09/04/2020 Time: 19:20:27 \n\nDear Sirs,\n \nPlease be advised that subject case is to be supplied by our end. Reverting with forwarding details."]
[null,null,null,null,10905,"103_30/3/2020 8:32:14 PM","2020-03-20","Defect","Owner / Marine / Tech. Suptd.","Engineering Audit","Kyma Shaft power KDU-110,\nZero calibration need to be performed at anchorage\n\n","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.15","Low","","","calibration carried out","2020-05-30","","Completed","2020-04-30","No","No","No","Internal"]
[null,null,null,null,10906,"103_30/3/2020 8:41:49 PM","2020-03-20","Defect","Owner / Marine / Tech. Suptd.","Engineering Audit","All computers:\nNeed to be secured all monitors, printer and CPUs. Also all associate cables need to be arranged properly and tie up with cables ties. Power trails to be secured properly\n\n\n\n","Miscellaneous","Communication","Equipment Related","","","","","all monitors, printer and CPUs secured. Also all associate cables need  arranged properly and tie up with cables ties. Power trails  secured properly\n\n","2020-04-30","","Completed","2020-04-15","No","No","No","Internal"]
[null,null,null,null,10907,"103_30/3/2020 8:51:53 PM","2020-03-20","Defect","Owner / Marine / Tech. Suptd.","Engineering Audit","VSAT and FBB installation: a) Both pedestals (VSAT and FBB) need to be painted b) VSAT rack to be secured properly.","Miscellaneous","Communication","Equipment Related","","","","","Both pedestals painted and VSAT rack secured.","2020-05-30","","Completed","2020-05-08","No","No","No","Internal","07-June-2020\nIs this is still not completed?"]
[null,null,null,null,10908,"103_30/3/2020 9:04:42 PM","2020-03-20","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Various installation:\nVarious cables laid at different places. All cable coaming to be filled up with approved electrical putty. All cables need to be arranged and secure properly\n\n\n\n","Miscellaneous","Communication","Equipment Related","","","","","All cable coamings filled up with approved putty. All cables securely arranged.","2020-04-30","","Completed","2020-04-05","No","No","No","Internal"]
[null,null,null,null,10909,"103_30/3/2020 9:42:11 PM","2020-03-20","Observation","Owner / Marine / Tech. Suptd.","Engineering Audit","ODME: ODME function and system to be tried out. Just to make system is working fine","Miscellaneous","MARPOL Related","Equipment Related","","","","","ODME function test carried out and alarms/trips tried out. Found satisfactory","2020-05-30","","Completed","2020-04-08","No","No","No","Internal"]
[null,null,null,null,10910,"103_30/3/2020 9:46:03 PM","2020-03-20","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","There are alarm for LOW ANODE / Anode alarm. Need to clean the strainers and inspect the condition of MGPS anodes and send us the photo. If anodes are worn out then raise RO","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","Anodes replaced with spare and fault rectified","2020-05-30","","Completed","2020-04-29","No","No","No","Internal"]
[null,null,null,null,10911,"103_30/3/2020 9:50:29 PM","2020-03-20","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","One pneumatic actuator for damper is removed and lying on incinerator top section. It seems some issue on damper side.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Received new dampers fixed in place and dampers made operational","2020-05-30","GILOS-077 Incinerator","Completed","2020-08-15","No","No","No","Internal","08-June-2020:\nThe spares are ready in Korea. The same was ordered to Yikang Marine."]
[null,null,null,null,10913,"103_30/3/2020 10:03:07 PM","2020-03-20","Observation","Owner / Marine / Tech. Suptd.","Engineering Audit","Emergency Switchboard: a) No.2 ER vent fan some of the aux contactors are chattering. Check aux contactor and overhaul if necessary. b) On Emergency Generator control panel section, Some of aux contactors are chattering. These aux contractors are need to be\n\n    overhauled.\n\nc) 220 volts earth meter showing slight low insulation, need to be \n\n    cleared. \n\n","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","contactor overhauled and working fine , insulation near to infinity","2020-05-30","","Completed","2020-04-20","No","No","No","Internal"]
[null,null,null,null,10914,"103_30/3/2020 10:06:03 PM","2020-03-20","Observation","Owner / Marine / Tech. Suptd.","Engineering Audit","Cable Coaming:Many places vessel has laid new cables, Many cable coamings cementing removed to pass the cables, ECR Console some of the cable coaming is not filled up with electrical putty. Approved type electrical putty to be filled up all coamings\n\n","Miscellaneous","General Appearance","Inappropriate Procedure","","","","","job completed electrical putty applied on comings as required","2020-04-30","","Completed","2020-04-18","No","No","No","Internal"]
[null,null,null,null,10915,"103_30/3/2020 10:09:04 PM","2020-03-20","Observation","Owner / Marine / Tech. Suptd.","Engineering Audit","Transas SSAS system: System to be installed and commissioning. DC power must be taken from GMDSS console DC 24 volts. Once installed follow up with office for testing. \n\n","Miscellaneous","Communication","Equipment Related","","","","","job completed and system tried out working satisfactory","2020-04-30","","Completed","2020-04-02","No","No","No","Internal"]
[null,null,null,null,10916,"103_30/3/2020 10:34:43 PM","2020-03-20","Defect","Ship Staff","Ship Staff Insp.","FWG  EJECTOR NO 1 PUMP SEAL LEAKING AND CASING HOLED","E/R - Aux. Mach.","General Appearance","Equipment Related","","","","","New pump received with motor same fixed in place and tested.","2020-05-30","GILOS - 024  FW GEN EJECTOR PUMP SPARES","Completed","2020-06-30","No","No","No","Internal"]
[null,null,null,null,10917,"103_30/3/2020 10:37:22 PM","2020-03-20","Defect","Ship Staff","Ship Staff Insp."," NO.2 M.C.S.W PUMP SEAL LEAK","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Seal replaced with received spare and leak rectified","2020-05-30","GILOS - 023 M.C.S.W Pump Spares","Completed","2020-06-24","No","No","No","Internal"]
[null,null,null,null,10918,"103_30/3/2020 10:40:52 PM","2020-03-20","Defect","Ship Staff","Ship Staff Insp."," NO.2 IG DECK SEAL PUMP SEAL LEAK","Cargo Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Mechanical seal replaced with received spare and leak rectified","2020-05-30","GILOS - 022  Deck Seal pump","Completed","2020-06-27","No","No","No","Internal"]
[null,null,null,null,10919,"103_30/3/2020 10:43:28 PM","2020-03-20","Other","Ship Staff","Ship Staff Insp.","ALL ER BILGE WELL CLEANING TO BE DONE.","Miscellaneous","General Appearance","Inappropriate Procedure","","","","","Scumming of oil and traces of oil removed with absorbent pads. No oil floating in bilge wells","2020-06-30","","Completed","2020-08-12","No","No","No","Internal"]
[null,null,null,null,10921,"103_30/3/2020 10:49:29 PM","2020-03-20","Critical Equipment","Ship Staff","Ship Staff Insp.","EMG FIRE PUMP STARTING DIFFICULT IN  BALLAST CONDITION. VACUUM UNIT NOT WORKING.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","","","","","Vacuum unit overhauled by shore workshop and made operational","2020-03-30","","Completed","2020-03-21","No","No","No","Internal"]
[null,null,null,null,10922,"103_30/3/2020 10:51:21 PM","2020-03-20","Defect","Ship Staff","Ship Staff Insp.","ME UNDER PISTON DOORS LEAKING.","E/R - Main Engine","Eng. / Strg. Comp.","Inappropriate Procedure","","","","","Unit #1, #5 & #6 leak rectified. Unit #2, #3, #4 rectification done. Testing for leak done during Main Engine operation","2020-05-30","","Completed","2020-08-21","No","No","No","Internal","08-June-2020:\nPlease update the latest status in this issue."]
[null,null,null,null,10923,"103_30/3/2020 10:53:13 PM","2020-03-20","Other","Ship Staff","Ship Staff Insp.","AE #1 DUE FOR DE CARB","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Decarb completed","2020-06-30","GILOS - 021 AE1 DECARB SPARES","Completed","2020-08-29","No","No","No","Internal"]
[null,null,null,null,10924,"103_30/3/2020 11:06:09 PM","2020-03-20","Other","Ship Staff","Ship Staff Insp.","FW TANK (STBD) WATER SALINITY IS HIGH","Miscellaneous","Eng. / Strg. Comp.","Inappropriate Procedure","","","","","Tank completely drained, cleaned and inspected. no abnormalities found in the tank and from adjacent bulk heads","2020-04-30","","Completed","2020-04-21","No","No","No","Internal"]
[null,null,null,null,10925,"103_30/3/2020 11:09:28 PM","2020-03-20","Defect","Owner / Marine / Tech. Suptd.","Engineering Audit"," BOILER  PANEL ALARM IS ON \" EMES BATTERY LOW\". NEW BATTERY TO ORDER AND CHECK\t\t\t\t\t\t\t\t\t\n\n","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","Battery replaced by service technician ","2020-05-30","","Completed","2020-04-25","No","No","No","Internal"]
[null,null,null,null,10926,"103_30/3/2020 11:16:05 PM","2020-03-20","Defect","Ship Staff","Ship Staff Insp."," NO.2 HFO PURIFIER  IS NOT OPERATIONAL.","E/R - Purifier","Eng. / Strg. Comp.","Equipment Related","","","","","No.2 HFO Purifier assembled and tested with FO feed. Found working satisfactorily. Testing for continous operation carried out","2020-05-30","","Completed","2020-07-12","No","No","No","Internal"]
[null,null,null,null,10927,"103_30/3/2020 11:20:29 PM","2020-03-20","Observation","Ship Staff","Ship Staff Insp."," NO.1 HFO PURIFIER STOPS EVERY 24 HRS WITH ALARM \"BOWL SPEED LOW\". AGAIN PURIFIER HAS TO BE RE STARTED.","E/R - Purifier","Eng. / Strg. Comp.","Equipment Related","","","","","Purifier now operational. No alarms","2020-04-30","","Completed","2020-04-10","No","No","No","Internal"]
[null,null,null,null,10928,"103_30/3/2020 11:22:28 PM","2020-03-20","Other","Ship Staff","Ship Staff Insp.","ER TANK TOP  AREA  TO CLEAN.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","Tank top area completely cleaned and rust marks touched up with paint","2020-04-30","","Completed","2020-04-25","No","No","No","Internal"]
[null,null,null,null,10929,"103_30/3/2020 11:26:05 PM","2020-03-20","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","IN GENERAL MOST OF THE PIPELINE  INSULATION  LAGGING IN BAD SHAPE. NEEDS TO BE REPLACED.\t\t\t\t\t\t\t\n\n\n\n","Miscellaneous","Eng. / Strg. Comp.","Inappropriate Procedure","","","","","Lagging replaced with spare supplied.","2020-04-30","","Completed","2020-04-20","No","No","No","Internal"]
[null,null,null,null,10930,"103_30/3/2020 11:30:10 PM","2020-03-20","Observation","Ship Staff","Ship Staff Insp.","ER TANK VENT HEADS ON DECK NEEDS TO BE CHECKED AND OVERHAULED AS REQUIRED","Miscellaneous","Eng. / Strg. Comp.","Inappropriate Procedure","","","","","Tank Heads inspected. Corroded plates fabricated and tank heads assembled back.","2020-05-30","","Completed","2020-05-11","No","No","No","Internal"]
[null,null,null,null,10931,"103_30/3/2020 11:32:00 PM","2020-03-20","Observation","Ship Staff","Ship Staff Insp.","SOME OF THE PRESSURE GAUGES AND THEROMETERS TO BE REPLACED.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","Pressure and thermometers replaced with spare received.","2020-05-30","","Completed","2020-04-20","No","No","No","Internal"]
[null,null,null,null,10932,"103_30/3/2020 11:34:46 PM","2020-03-20","Defect","Ship Staff","Ship Staff Insp.","BOTH MAIN AIR RESERVIOUR AUTO DRAIN  NOT WORKING.","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related","","","","","Both auto-drain pot were removed cleaned and inspected. Now are working satisfactory.","2020-10-30","","Completed","2020-10-30","No","No","No","Internal","07-Jun-2020:\nPlease advise if any requisition has been raised for same?\n\n\nPlease update, if the same has been rectified, Till that time, please drain the air bottle every watch."]
[null,null,null,null,10933,"103_30/3/2020 10:56:06 PM","2020-03-20","Observation","Ship Staff","Ship Staff Insp.","MINERALIZER NOT WORKING.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","Dolomite received filled up in the mineralizer and made operational","2020-05-30","","Completed","2020-04-27","No","No","No","Internal"]
[null,null,null,null,10934,"103_30/3/2020 11:46:55 PM","2020-03-20","Observation","Ship Staff","Ship Staff Insp.","INCINERATOR WASTE OIL TANK / SAVE ALL TRAYS TO BE CLEANED.","Miscellaneous","Eng. / Strg. Comp.","Inappropriate Procedure","","","","","Incinerator Waste oil save all trays cleaned and painted","2020-04-30","","Completed","2020-04-15","No","No","No","Internal"]
[null,null,null,null,10935,"103_31/3/2020 12:03:47 AM","2020-03-20","Observation","Ship Staff","Ship Staff Insp.","ME FUEL VALVE TESTING DEVICE OPERATIONAL IS SLUGGISH","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","Reconditioned Fuel valve testing machine received","2020-05-30","GILOS - 015 FUEL VALVE TESTING DEVICE","Completed","2020-08-22","No","No","No","Internal","New  Fuel Valve testing machine has been ordered by GW."]
[null,null,null,null,10937,"103_31/3/2020 6:54:27 AM","2020-03-20","Defect","Ship Staff","Ship Staff Insp.","HYDRAULIC LINES FOR MOORIN WINCHES CONTROL LEVER AND REMOTE CONTROL FOUND WASTED AND HEAVILY CORRODED","Deck - Pipe / Fittings","Mooring","Equipment Related,Inappropriate Procedure","","","","","VESSEL RECEIVED SPARE PIPELINES AND ALSO BLANKED THE SECTION OF PIPELINES TO AVOID LEAKAGES DURING NORMAL OPERATION.","2020-06-20","GILO200060","Completed","2020-06-11","No","No","No","Internal","07-June-2020:\nAs discussed - the remote operation line for the mooring winch line is to be blanked. Please advise if all remote operation line for the mooring winch line has been blanked by now."]
[null,null,null,null,10942,"103_30/3/2020 11:38:48 PM","2020-03-20","Other","Ship Staff","Ship Staff Insp.","AIR COMPRESSOR SAVE ALL TRAYS NOTICED WITH OIL AND WATER AT ALL TIMES.\t\t\t\t\t\n\n\n\n","E/R - Air Comp.","Eng. / Strg. Comp.","Inappropriate Procedure","","","","","Leak from LO filters and cooling water line rectified","2020-05-30","","Completed","2020-04-20","No","No","No","Internal"]
[null,null,null,null,11469,"103_1/4/2020 3:47:27 AM","2020-03-20","Observation","Ship Staff","Nav Audit / Verification","Echo sounder repeater unit dimmer switch not operational.","Navigation - Echo Sounder / Speed Log","Navigation","Equipment Related","","","","","SAME REAPIRED TESTED WORKING SATISFACTORY","2020-04-15","","Completed","2020-05-06","No","No","No","Internal"]
[null,null,null,null,11470,"103_1/4/2020 3:50:32 AM","2020-03-20","Observation","Ship Staff","Ship Staff Insp.","Clinometer dimmer switch not operational.","Navigation - Others","Navigation","Equipment Related","","","","","SAME RECTIFIED WORKING SATISFACTORY","2020-04-15","","Completed","2020-05-06","No","No","No","Internal"]
[null,null,null,null,10982,"103_31/3/2020 5:56:30 AM","2020-03-20","Defect,Observation","Ship Staff","Ship Staff Insp.","BOTH LIFEBOAT GRIPES FOUND WASTED","LSA / FFA","Safety / LSA / FFA","Human Error,Inappropriate Procedure","","","","","NEW GRIPES RECEIVED AND RENEWED","2020-04-30","","Completed","2020-03-30","No","No","No","Internal"]
[null,null,null,null,11530,"103_30-Apr-20 9:00:30 PM","2020-03-21","Defect","Ship Staff","Ship Staff Insp.","#1 AHU leak","Accommodation","Eng. / Strg. Comp.","Equipment Related","","","","","Leak testing done by shore technicians and found no leak in AHU. Leak from the compressor unloaders","2020-05-30","GILOS - 052 AIR HANDLING UNIT","Completed","2020-08-20","No","No","No","Internal"]
[null,null,null,null,11560,"103_30/4/2020 4:32:07 PM","2020-03-21","Defect,Observation","Ship Staff","Ship Staff Insp.","Lifebouy's found defected and damaged.","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","Requisition raised for new lifebouys. ","2020-03-30","","Completed","2020-03-29","No","No","No","Internal"]
[null,null,null,null,10896,"103_30/3/2020 11:36:49 PM","2020-03-21","Defect","Ship Staff","Ship Staff Insp.","EGB DIFF MANOMETER IS DEFECTIVE.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","Line cleared and liquid filled in the manometer","2020-05-30","","Completed","2020-04-03","No","No","No","Internal"]
[null,null,null,null,10938,"103_30/3/2020 9:22:32 PM","2020-03-21","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","SAAB system fail alarm coming frequently and getting reset by it self","Miscellaneous","Cargo / Ballast Systems","Equipment Related","","","","","time delay of the alarm increased as per office instructions and continuos monitoring in progress.","2020-05-30","","Completed","2020-04-20","No","No","No","Internal"]
[null,null,null,null,10939,"103_30/3/2020 9:25:55 PM","2020-03-21","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","SAAB system fail alarm coming frequently and getting reset by it self","Elect. Mach. & Equip.","Cargo / Ballast Systems","Equipment Related","","","","","time delay of the alarm increased as per office instructions and continuos monitoring in progress.","2020-05-30","","Completed","2020-04-20","No","No","No","Internal"]
[null,null,null,null,10940,"103_30/3/2020 9:35:39 PM","2020-03-21","Defect","Owner / Marine / Tech. Suptd.","Engineering Audit","No.2 Cargo Oil Strip educator gauges in CCR are not showing correct. Need to calibrate and see further. Also make sure in PR side control air to controller are getting correct pressure. No water in control line, Drain the line, clear the flapper and filter on controller and see whether gauges shows correct reading","Deck - Machinery","General Appearance","Equipment Related","","","","","job completed and checked gauges at all locations working satisfactory","2020-05-30","","Completed","2020-04-21","No","No","No","Internal"]
[null,null,null,null,10943,"103_30/3/2020 11:18:37 PM","2020-03-21","Defect","Ship Staff","Ship Staff Insp.","NO.1 BOILER F.O. PUMP SEAL LEAK.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","New pump supplied and fitted in place of #2 Boiler FO pump. Seal leaked during first start. Spare seals received for the newly installed pump","2020-05-30","","Completed","2020-08-15","No","No","No","Internal","Noted on same, Owners are trying to arrange the SE to rectify the same."]
[null,null,null,null,10944,"103_30/3/2020 11:40:51 PM","2020-03-21","Observation","Ship Staff","Ship Staff Insp.","SEWAGE TRETAMENT PLANT SLUDGE RETURN PIPE IS OPAQUE. DIFFICULT TO SEE THE FLOW","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","STP cleaned and sludge return activated. Sludge return pipe replaced with received spare.","2020-05-30","GILOS - 070 SEWAGE TREATMENT PLANT","Completed","2020-06-29","No","No","No","Internal"]
[null,null,null,null,10945,"103_30/3/2020 11:24:10 PM","2020-03-21","Observation","Owner / Marine / Tech. Suptd.","Engineering Audit","  ECR  MAIN SWITHCBOARD  INSULATION MAT  CERTIFICATE IS MISSING. ","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","SWITHCBOARD  INSULATION MAT REPLACED WITH SPARE AND  CERTIFICATE POSTED ON SWITCHBOARD","2020-05-30","","Completed","2020-04-22","No","No","No","Internal"]
[null,null,null,null,10946,"103_30/3/2020 11:43:12 PM","2020-03-21","Defect","Ship Staff","Ship Staff Insp.","INCINERATOR  SECONDARY COMBUSTION CHAMBER REFRACTORY TO BE REPAIR","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","Refractory patched up in damaged areas","2020-05-30","","Completed","2020-04-29","No","No","No","Internal"]
[null,null,null,null,10947,"103_30/3/2020 11:44:48 PM","2020-03-21","Observation","Ship Staff","Ship Staff Insp.","ER VENTILATION DUCTS TO BE CLEANED","Miscellaneous","Eng. / Strg. Comp.","Inappropriate Procedure","","","","","Cleaning and painting of ducts completed","2020-05-30","","Completed","2020-06-17","No","No","No","Internal"]
[null,null,null,null,10948,"103_31/3/2020 12:08:20 AM","2020-03-21","Critical Equipment","Owner / Marine / Tech. Suptd.","Engineering Audit","SMOKE DETECTOR ABOVE BOILER IS  NOT OPERATIONAL.  IN GENERAL ALL DETCTOR HEADS TO BE CHECKED AS SOME OF THEM TIED WITH TAPE","Critical Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","Complete fire detection system upgraded and all FD,SD, TD and MCP renewed","2020-05-30","GILOS - 017 FIRE DETECTOR HEAD","Completed","2020-08-20","No","No","No","Internal","Complete Fire Alarm Panel is being upgraded now. Mr. Kamlesh is following with Martek Singapore."]
[null,null,null,null,10949,"103_31/3/2020 12:11:34 AM","2020-03-21","Other","Ship Staff","Ship Staff Insp.","ER SPARES NOT ARRANGED AND FOUND MIXED UP.  NO INVENTORY MAINTAINED. SAME TO BE ARRANGED AFTER TAKING INVENTORY","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","Spares arranged, inventory taken and cleaning of spare store and painting completed.","2020-05-30","","Completed","2020-05-27","No","No","No","Internal"]
[null,null,null,null,10950,"103_31/3/2020 12:15:00 AM","2020-03-21","Defect","Ship Staff","Ship Staff Insp.","ME JACKET WATER CONTROLLER NOT WORKING. TEMP BEING ADJUSTED MANUALLY.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Renewed with spare recvied controller. ","2020-05-30","GILO200045 -  Temperature Controller for M/E Jacket Cooling water system","Completed","2020-09-30","No","No","No","Internal","07-Jun-2020\nThe same has been ordered to Yikang  on 05-June 2020."]
[null,null,null,null,10951,"103_31/3/2020 12:25:23 AM","2020-03-21","Observation","Ship Staff","Ship Staff Insp.","AUX ENGINES LOOKS DIRTY WITH STAINS OF OIL AND WATER.","E/R - Aux. Engine","Eng. / Strg. Comp.","Inappropriate Procedure","","","","","Cleaning of AE's done. Leaks from crankcase door rectified","2020-04-30","","Completed","2020-04-22","No","No","No","Internal"]
[null,null,null,null,10952,"103_31/3/2020 12:27:41 AM","2020-03-21","Observation","Ship Staff","Ship Staff Insp.","ALL ELECTICAL LOCAL PANELS  FOUND RUSTED AND INNER SURFACE LOOKS DUSTY.\n\n","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Inappropriate Procedure","","","","","ALL ELECTICAL LOCAL PANELS   CLEANING CARRIED OUT , INNER SURFACE CLEANED WITH AIR ","2020-05-30","","Completed","2020-05-25","No","No","No","Internal"]
[null,null,null,null,10953,"103_31/3/2020 12:37:47 AM","2020-03-21","Defect","Ship Staff","Ship Staff Insp.","MAIN ENGINE #3 FUEL INJECTOR LEAK","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Leak from return line of Fuel injector rectified","2020-04-30","","Completed","2020-04-15","No","No","No","Internal"]
[null,null,null,null,10954,"103_31/3/2020 12:40:08 AM","2020-03-21","Defect","Ship Staff","Ship Staff Insp.","EGB MANOMETER NOT WORKING","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","Manometer lines cleared and liquid filled","2020-05-30","","Completed","2020-04-10","No","No","No","Internal"]
[null,null,null,null,10957,"103_31/3/2020 12:51:10 AM","2020-03-21","Defect","Ship Staff","Ship Staff Insp.","BILGE PUMP TO BE OVERHAULED","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","","","","","Spares received. Overhauling of pump done. Pump in complete operation","2020-05-30","","Completed","2020-08-04","No","No","No","Internal","Vessel overhauled this pump, however spares are required."]
[null,null,null,null,10958,"103_31/3/2020 12:53:49 AM","2020-03-21","Observation","Ship Staff","Ship Staff Insp.","MAIN STEAM VALVE FOR #2 BOILER TO BE FREED","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","Stem stop valve opened up from bonnet, jacked and freed up","2020-05-30","","Completed","2020-04-25","No","No","No","Internal"]
[null,null,null,null,10959,"103_31/3/2020 12:57:25 AM","2020-03-21","Defect","Ship Staff","Ship Staff Insp.","POWER PACK AFT AIR REGULATOR AND FILTER LEAKING","Deck - Machinery","Eng. / Strg. Comp.","Equipment Related","","","","","AIR REGULATOR AND AIR FILTER REPLACED WITH NEW SPARE","2020-05-30","","Completed","2020-04-26","No","No","No","Internal"]
[null,null,null,null,11471,"103_1/4/2020 5:50:25 AM","2020-03-21","Observation","Ship Staff","Ship Staff Insp.","SAFETY WALKWAY CHAIN FOUND HEAVILY CORRODED AND WASTED","Hull & Tanks","Structural Condn. / WT integrity ","External Factors","","","","","SAFETY WALKWAY CHAINS RENEWED WITH NEW CHAIN AND NOW ALL IN PLACE.","2020-04-30","","Completed","2020-04-26","No","No","No","Internal"]
[null,null,null,null,11472,"103_1/4/2020 6:00:44 AM","2020-03-21","Observation","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","REQUIRED LENGTH OF HOSE FOR MEASURING TOXIC GASES INSIDE CARGO/BALLAST TANK NOT AVAILABLE ON BOARD FOR GASTEC PUMP.","Miscellaneous","Cargo / Ballast Systems","Equipment Related,Inappropriate Procedure","5.23","Very High","","","NEW HOSE RECEIVED.","2020-06-20","GILO200001","Completed","2020-04-08","No","No","No","External"]
[null,null,null,null,10961,"103_31/3/2020 1:02:53 AM","2020-03-21","Defect","Ship Staff","Ship Staff Insp.","MAIN AIR COMP NO 2 NOT PUMPING","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related","","","","","1st stage suction valve securing nut found slack. Head lifter up and valve replaced with overhauled spare","2020-05-30","","Completed","2020-04-01","No","No","No","Internal"]
[null,null,null,null,10962,"103_31/3/2020 12:33:22 AM","2020-03-21","Defect","Ship Staff","Ship Staff Insp.","MAIN AIR COMP NO 2 AMPS NEEDLE MISSING","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related","","","","","Amp meter replaced with spare , tested working satisfactory","2020-05-30","GILOS - 046 - AMPERE METER FOR VARIOUS MOTORS","Completed","2020-06-25","No","No","No","Internal","07-June-2020\nThis is ordered and ready for delivery. The spares are ready in Singapore."]
[null,null,null,null,10965,"103_31/3/2020 1:14:07 AM","2020-03-21","Defect","Owner / Marine / Tech. Suptd.","Engineering Audit","220 VOLT LOW INSULATION ALL WIRING MELTED IN LIGHTNING","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","INSULATION SLEEVE FITTED AND WIRING RENEWED AS REQUIRED","2020-05-30","","Completed","2020-04-20","No","No","No","Internal"]
[null,null,null,null,10966,"103_31/3/2020 1:18:16 AM","2020-03-21","Defect","Ship Staff","Ship Staff Insp.","SERVICE AIR BOTTLE MANHOLE GASKET LEAKING","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related","","","","","Gasket replaced and leak rectified","2020-05-30","","Completed","2020-04-14","No","No","No","Internal"]
[null,null,null,null,10967,"103_31/3/2020 6:45:41 AM","2020-03-21","Observation","Ship Staff","Ship Staff Insp.","FRESH WATER LINE ON DECK FOUND LEAKING FROM MANY FLANGES","Deck - Pipe / Fittings","Cargo / Ballast Systems","External Factors","","","","","ALL LEAKING FLANGE GASKETS RENEWED, LINE TESTED.","2020-06-21","","Completed","2020-05-05","No","No","No","Internal"]
[null,null,null,null,10968,"103_31/3/2020 6:48:15 AM","2020-03-21","Defect","Ship Staff","Ship Staff Insp.","THE HYDRAULIC RETURN LINE ON PORT AND STBD WINDLASS FOUND HEAVILY CORRODED AND WASTED","Deck - Mooring Machinery","Mooring","Equipment Related,Inappropriate Procedure","","","","","SPARE FLEXIBLE HOSES AVAILABLE ONBOARD FOR RENEWAL IN CASE OF EMERGENCY. CURRENTLY NO LEAKAGES OBSERVED AND PIPES FOUND INTACT. KINDLY ADVISE IF THIS ITEM CAN BE SHIFTED TO COMPLETED LIST","2020-06-21","","Completed","2020-06-13","No","No","No","Internal"]
[null,null,null,null,11531,"103_30-Apr-20 9:30:01 PM","2020-03-22","Critical Equipment","Ship Staff","Ship Staff Insp.","FIXED FOAM SYSTEM TANK LEVELS LOW","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","FOAM RECIEVED AND REFILLED","2020-05-10","GILO200006","Completed","2020-06-21","No","No","No","Internal","Low Expansion foam will be supplied by owners in Ningbo.\nHigh Expansion foam will be supplied by GW in Singapore"]
[null,null,null,null,11561,"103_30-Apr-20 8:50:35 PM","2020-03-22","Observation","Ship Staff","Ship Staff Insp.","FORWARD EMERGENCY EMBARKATION PORTABLE LIGHT FOR LIFERAFT NOT WORKING","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","REQUISITION RAISED","2020-04-24","","Completed","2020-04-08","No","No","No","Internal"]
[null,null,null,null,11562,"103_30-Apr-20 9:34:20 PM","2020-03-22","Observation","Ship Staff","Ship Staff Insp.","PORTABLE FIRE EXTINGUISHER SPARE FOAM CONCENTRATE NOT AS PER REQUIREMENT","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","REQUISITION RAISED","2020-04-30","GILO205085","Completed","2020-04-08","No","No","No","Internal"]
[null,null,null,null,11473,"103_1/4/2020 3:43:02 AM","2020-03-22","Observation","Ship Staff","Nav Audit / Verification","SAT-C, Unable to Log in/out. Unable to change region, unable to carry out PV test.","Navigation - GMDSS & Communication","Communication","Equipment Related","","","","","Assistance from office/Technician received, system working , AFTER ONE WEEK SYSTEM AGAIN DOWN AND ANTEENA REPLACED , PRESENTLY WORKING SATISFACTORY","2020-04-15","","Completed","2020-03-27","No","No","No","Internal"]
[null,null,null,null,10969,"103_30/3/2020 9:12:55 PM","2020-03-22","Observation","Owner / Marine / Tech. Suptd.","Engineering Audit","IT stores: Proper IT stores to be made and keep all IT items at one place. Make inventory for record \n\n","Elect. Mach. & Equip.","General Appearance","Inappropriate Procedure","","","","","IT STORE ARRANGED ","2020-05-30","","Completed","2020-04-12","No","No","No","Internal"]
[null,null,null,null,10970,"103_30/3/2020 11:48:28 PM","2020-03-22","Observation","Ship Staff","Ship Staff Insp.","INCINERATOR SLUICE DOOR OPENING IS SLUGGISH.  HAND HAMMER USED TO OPEN THE DOOR.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Inappropriate Procedure","","","","","Spare received. Dampers fixed and made operational","2020-05-30","GILOS - 077 INCINERATOR","Completed","2020-08-15","No","No","No","Internal","14-May-2020\nPlease arrange to provide Gilos with GILO205123 from Yikang as per their offer for $1,662.05 USD."]
[null,null,null,null,11545,"103_1/5/2020 5:31:53 AM","2020-03-23","Observation","Ship Staff","Ship Staff Insp.","The UTIs and Sounding rod on board are not of enclosed type for use on tankers and possess risk of exposure to harmful gases during gauging and sounding of cargo tanks","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","1 UTI recieved after shore repairs and calibration. Other acceptable on tankers as per office communication.","2020-07-23","","Completed","2020-06-22","No","No","No","Internal","28-May-2020:\nDear Captain Ajay\n \nUnits with Serial Nos R12135 & R10578 are the latest version of Enraf Tanksystem’s Utimeter  Restricted (open) type Units. In order to confirm Serial Nos please find a picture showing how to locate them."]
[null,null,null,null,11474,"103_1/4/2020 4:10:38 AM","2020-03-23","Observation","Ship Staff","Ship Staff Insp.","Rpm repeater on STBD bridge wing showing error. Engine stopped repeater showing ahead 45 Rpm.","Navigation - Others","Navigation","Equipment Related","4.7","High","","","RPM INDICATOR ON STBD BRIDGE WING, REPLACED WORKING SATISFACTORY.","2020-04-10","GILO200018","Completed","2020-08-26","No","No","No","Internal","05-June-2020:\nDear Mr. Christos,\n\nPlease find quotation from maker for Bridge Wing RPM Indicator. Please approve. \n\nThis is required to clear below defect:\n+++\nRpm repeater on STBD bridge wing showing error. Engine stopped repeater showing ahead 45 Rpm.\n+++"]
[null,null,null,null,10972,"103_31/3/2020 6:42:49 AM","2020-03-23","Critical Equipment,Observation","Ship Staff","Ship Staff Insp.","BOTH HOSE HANDLING CRANES HOSES FOUND LEAKING FROM THE BLOCK","Deck - Machinery","Cargo / Ballast Systems","Equipment Related","","","","","BOTH HH CRANE WINCH BLOCK REPLACED WITH NEW SPARE RECEIVED AND LEAK RECTIFIED","2020-06-23","GILO205112","Completed","2020-08-18","No","No","No","Internal","Please mention PO number ( GILOS - 071- 2020). we are sourcing suitable quotation and will revert soonest possible.\n\n14-May-2020:\nDear Sirs,\n \nPlease be advised that due to poor condition of both Hose Handling Cranes winches the entire GILO205112 has been approved and is to be delivered on board the soonest.\n \nNote that delivery time is 4 weeks from suppliers."]
[null,null,null,null,10973,"103_31/3/2020 6:18:55 AM","2020-03-24","Breakdown,Defect","Ship Staff","Ship Staff Insp.","NO.3 MANIFOLD VALVE ON PORT SIDE FOUND STUCK IN CLOSED CONDITION. THE VALVE SPINDLE IS TURNING FREELY","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","","","","","ACTUATOR RECEIVED AND FITTED IN POSITION. VALVE OPERATION IS SATISFACTORY.","2020-06-24","GILO205078","Completed","2020-06-22","No","No","No","Internal","The one supplied by GW turned out to be unsuitable. The same will be returned back to Supplier.\n\nNext One will be supplied Owners directly"]
[null,null,null,null,10974,"103_31/3/2020 6:26:41 AM","2020-03-24","Observation","Ship Staff","Ship Staff Insp.","NO.2 MANIFOLD VALVE ON PORT SIDE FOUND VERY HARD TO OPERATE","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","","","","","WORM GEAR INSPECTED AND FOUND FROZEN. SAME GREASED AND FREED. VALVE NOW FREE TO OPERATE","2020-06-24","","Completed","2020-04-21","No","No","No","Internal"]
[null,null,null,null,10975,"103_31/3/2020 6:56:52 AM","2020-03-24","Observation","Ship Staff","Ship Staff Insp.","DEADMAN ROLLER AND GUIDE ROLLER ON FOCSLE DECK FOUND FROZEN AND HEAVILY RUSTED","Deck - Pipe / Fittings","Mooring","Equipment Related,External Factors","","","","","ROLLERS GREASED AND FREED UP ","2020-06-24","","Completed","2020-04-30","No","No","No","Internal"]
[null,null,null,null,11532,"103_30/4/2020 11:51:22 AM","2020-03-25","Observation","Ship Staff","Ship Staff Insp.","AUX. ENGINE #2 LUBE OIL TEMPERATURE SENSOR NOT OPERATIONAL","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","SENSOR REPLACED WITH SPARE AND TESTED WORKING SATISFACTORY","2020-05-30","GILOS - 029  AUX. ENGINE LUBE OIL TEMPERATURE SENSOR","Completed","2020-07-02","No","No","No","Internal","Same is approved for supply and it will take another 45 days for the same to be ready."]
[null,null,null,null,11555,"103_1/5/2020 7:08:05 AM","2020-03-26","Observation","Ship Staff","Ship Staff Insp.","DURING CARGO OPERATIONS IT WAS OBSERVED THAT MANY CARGO TANKS POTENTIOMETER SHOWING ERRATIC READING","Cargo Mach.","Cargo / Ballast Systems","External Factors","","","","","THE VALVES TRIED OUT AND INDICATION MATCHED LOCALLY AND IN CCR ALSO. ADJUSTMENT DONE ON THE SUSPECTED VALVES AFTER VERIFYING THEIR STATUS PHYSICALLY (PUMPROOM VALVES). NOW ALL VALVES INDICATION IN CCR MATCHING WITH THE LOCAL INDICATION.","2020-07-26","","Completed","2020-05-26","No","No","No","Internal","Please advise, what is progress in this regard."]
[null,null,null,null,10976,"103_30/3/2020 11:03:41 PM","2020-03-30","Defect","Ship Staff","Ship Staff Insp.","STERLIZER NOT WORKING.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","UV LAMP AND BALAST REPLACED WITH SPARE AND SYSTEM TRIED OUT WORKING IN GOOD ORDER","2020-05-30","GILOS - 020 STERLIZER SPARES","Completed","2020-07-06","No","No","No","Internal","Approved to be supplied by Owners"]
[null,null,null,null,10977,"103_30/3/2020 11:52:22 PM","2020-03-30","Defect","Ship Staff","Ship Staff Insp.","PNEUMATIC HIGH PRESSURE PUMP FOR HYDRAULIC JACKS NOT WORKING.\t\t\t\t\t\t\t\t\t\n\n","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","New High pressure pump received","2020-05-30","","Completed","2020-04-22","No","No","No","Internal"]
[null,null,null,null,10978,"103_31/3/2020 12:18:30 AM","2020-03-30","Observation","Ship Staff","Ship Staff Insp.","FRESH WATER GENERATOR FOUND OPERATING IN LESS CAPACITY","Miscellaneous","Eng. / Strg. Comp.","Inappropriate Procedure","","","","","#1 FWG is in operation for water production with steam. Retubing of #1 FWG by shore workshop done and production increased.","2020-05-30","","Completed","2020-06-30","No","No","No","Internal","vessel is running #1 FWG and is trying to drill out the  choked pipe for FWG#2"]
[null,null,null,null,10979,"103_31/3/2020 12:21:00 AM","2020-03-30","Other","Ship Staff","Ship Staff Insp.","FEW OF THE ME SPECIAL TOOLS FOUND MISSING. (FOR EXAMPLE, STARTING AIR VALVE LAPPING TOOL, FUEL VALVE OVERHAUL TOOLS ETC)","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","Missing tools scattered in ER arranged in the tools board.","2020-05-30","","Completed","2020-05-09","No","No","No","Internal","Please advise if the requisition is raised for the missing Tools?"]
[null,null,null,null,10980,"103_31/3/2020 12:23:16 AM","2020-03-30","Observation","Ship Staff","Ship Staff Insp.","ER FIRE DAMPERS REQUIRED  DE RUSTING AND PAINTING.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","DERUSTING AND PAINTING CARRIED OUT.","2020-05-30","","Completed","2020-05-12","No","No","No","Internal","Please advise progress."]
[null,null,null,null,10981,"103_31/3/2020 1:07:29 AM","2020-03-30","Defect","Ship Staff","Ship Staff Insp.","MAIN ENGINE SOOT BLOWER PORT SIDE LEAKING TO BE RECTIFIED","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","Leak from gland packing rectified by changing the complete gland packing","2020-05-30","","Completed","2020-04-07","No","No","No","Internal"]
[null,null,null,null,11533,"103_30/4/2020 2:19:06 PM","2020-04-04","Defect","Ship Staff","Ship Staff Insp.","AMPERE METER FOR VARIOUS MOTORS ARE NOT OPERATIONAL","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.7","Medium","","","REPLACE WITH SPARES AND TESTED WORKING SATISFACTORY","2020-05-30","GILOS - 046 - AMPERE METER FOR VARIOUS MOTORS","Completed","2020-07-05","No","No","No","Internal","13-April-2020: Ordered to Martek Marine\n\nGood day Ms. Kamali, \n \nPlease proceed with the order.\n \nKindly note our official PO GILO205084 as per your below quotation PO AMOUNT: SGD 210.00/-"]
[null,null,null,null,11546,"103_1/5/2020 5:37:14 AM","2020-04-04","Observation","Ship Staff","Ship Staff Insp.","5C and 5S Cago tanks PV Valve found leaking","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","","","","","OVERHAULING CARRIED OUT. NO LEAKAGES OBSERVED.","2020-07-03","","Completed","2020-05-28","No","No","No","Internal","Please attend this on priority basis as this may cause rejection in terminal."]
[null,null,null,null,11540,"103_1/5/2020 4:50:36 AM","2020-04-05","Observation","Ship Staff","Ship Staff Insp.","Safety walkway chain found heavily corroded and wasted.","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","External Factors","","","","","Safety Walkway chains renewed","2020-05-31","","Completed","2020-04-26","No","No","No","Internal","Please confirm if the same is completed"]
[null,null,null,null,11559,"103_1/5/2020 7:22:49 AM","2020-04-05","Observation","Ship Staff","Ship Staff Insp.","Galley and pantry drains found choked","Accommodation","General Appearance","External Factors","","","","","All drains cleared.","2020-07-05","","Completed","2020-05-09","No","No","No","Internal","Please confirm that all drains are now clear."]
[null,null,null,null,11557,"103_1/5/2020 7:18:13 AM","2020-04-06","Observation","Ship Staff","Ship Staff Insp.","Weathertight doors on sunken and upper deck found not closing properly","Accommodation","ISPS Related","External Factors","","","","","All doors adjusted and dog legs freed","2020-07-06","","Completed","2020-05-12","No","No","No","Internal"]
[null,null,null,null,11558,"103_1/5/2020 7:20:21 AM","2020-04-06","Observation","Ship Staff","Ship Staff Insp.","Many fire doors in accommodation found not closing properly","Accommodation","Safety / LSA / FFA","External Factors","","","","","All fire doors adjusted for proper closure.","2020-07-06","","Completed","2020-05-23","No","No","No","Internal","Please advise progress in this regard."]
[null,null,null,null,11563,"103_30-Apr-20 8:29:20 PM","2020-04-07","Observation","Ship Staff","Ship Staff Insp.","Fire and foam  hydrants leaking.","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","Lapping of Fire and foam hydrants carried.","2020-04-25","","Completed","2020-04-23","No","No","No","Internal"]
[null,null,null,null,11548,"103_1/5/2020 5:45:13 AM","2020-04-08","Observation","Ship Staff","Ship Staff Insp.","The condition of walkie talkies onboard is not good and needs renewal especially the batteries. The reception and transmission is poor and causes difficulties during critical operations such as mooring and cargo operations","Miscellaneous","Communication","Equipment Related,Inappropriate Procedure","","","","","Received spares and new walkie talkies.","2020-07-07","GILO200004, GILO200005","Completed","2020-06-22","No","No","No","Internal","GILO200004, GILO200005 approved for supply,\n\n14-May-2020:\nGood day Capt. Ajay Chauhan,\n\nPlease note we had closed GILO205083. \n\nHowever, GILO200004 & GILO200005 will be supplied."]
[null,null,null,null,11551,"103_1/5/2020 6:10:57 AM","2020-04-08","Critical Equipment,Observation","Ship Staff","Ship Staff Insp.","None of the mooring winches and windlasses found greased\t","Deck - Mooring Machinery","Mooring","Behaviour Based,Human Error","","","","","Thourough greasing of all mooring winches, windlass carried out.","2020-07-07","","Completed","2020-04-27","No","No","No","Internal"]
[null,null,null,null,11564,"103_30-Apr-20 8:39:23 PM","2020-04-08","Observation","Ship Staff","Ship Staff Insp.","FIRE AND FOAM ISOLATION VALVES FROZEN.","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","FOAM AND FIRE ISOLATION VALVE LUBRICATION  CARRIED OUT.","2020-04-25","","Completed","2020-04-22","No","No","No","Internal"]
[null,null,null,null,11565,"103_1/5/2020 5:01:14 AM","2020-04-08","Breakdown,Critical Equipment","Ship Staff","Ship Staff Insp.","Port side pilot ladder extension rope parted while rigging up the combination ladder for pilot boarding.\t","Miscellaneous","Safety / LSA / FFA","External Factors","","","","","New pilot ladder installed with new extension rope as the pilot ladder also found manually hand spliced.","2020-04-30","","Completed","2020-04-15","No","No","No","Internal"]
[null,null,null,null,11568,"103_1/5/2020 5:14:44 AM","2020-04-08","Observation","Ship Staff","Ship Staff Insp.","Aft mooring rollers found frozen\t","Deck - Pipe / Fittings","Mooring","Behaviour Based,Inappropriate Procedure","","","","","All rollers lubed, freed, greased and made free to rotate","2020-05-30","","Completed","2020-04-26","No","No","No","Internal"]
[null,null,null,null,11539,"103_1/5/2020 4:43:25 AM","2020-04-09","Defect","Ship Staff","Ship Staff Insp.","The lever for testsing the COTs overfill alarm found frozen for all COTs\t\t\t","Hull & Tanks","Cargo / Ballast Systems","External Factors","","","","","While testing, same was freed and lubricated. Oiled and derusted again during next testing","2020-07-09","","Completed","2020-05-02","No","No","No","Internal"]
[null,null,null,null,11543,"103_1/5/2020 5:22:19 AM","2020-04-09","Observation","Ship Staff","Ship Staff Insp.","One of the manifold grating on port side found damaged\t","Deck - Pipe / Fittings","General Appearance","Human Error","","","","","Grating renewed","2020-05-30","","Completed","2020-05-02","No","No","No","Internal"]
[null,null,null,null,11556,"103_1/5/2020 7:11:44 AM","2020-04-12","Observation","Ship Staff","Ship Staff Insp.","NO.2 CARGO EDUCTOR GAUGES SHOWING ERRATIC READINGS, OBSERVED DURING CARGO DISCHARGING","Miscellaneous","Cargo / Ballast Systems","Equipment Related,Inappropriate Procedure","","","","","All lines cleared and gauges calibrated and adjusted. No.2 eductor Driving gauge has an error of -2.5 bars in pumproom.","2020-07-12","","Completed","2020-05-20","No","No","No","Internal","Please update progress in this issue."]
[null,null,null,null,11883,"103_13/5/2020 12:27:46 AM","2020-04-13","Defect","Ship Staff","Ship Staff Insp.","#1 Main Air Bottle Safety-Relief Valve leaking and outlet found blanked.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Relief valve replaced with new received spare.","2020-05-31","GILOS - 057 AIR RESERVOIR SAFETY-RELIEF VALVE","Completed","2020-08-02","No","No","No","Internal","22-April-2020: angie.tan@dintec.com.sg; service@dintec.com.sg,\n\nDear Mr. Upkar,\n\nWell received the purchase order GILO205099 for Vessel GILOS with many thanks and will proceed the order accordingly.\n\nThanks and best regards,"]
[null,null,null,null,11566,"103_1/5/2020 5:04:13 AM","2020-04-14","Breakdown,Critical Equipment","Ship Staff","Ship Staff Insp.","The shifting wire for starboard gangway parted while rigging\t","Miscellaneous","Safety / LSA / FFA","Inappropriate Procedure","","","","","Wire renewed with spare ones and greased","2020-04-30","","Completed","2020-04-29","No","No","No","Internal"]
[null,null,null,null,11570,"103_1/5/2020 4:47:55 AM","2020-04-15","Defect,Observation","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","No.2 COP Suction gauge showing erratic reading in CCR, locally and pumproom\t\t","Cargo Mach.","Cargo / Ballast Systems","Behaviour Based,Human Error","","","","","The valve was found closed and minor leakages observed from the connection at the pump side. Same was opened and rectified. Pressure gauge checked during cargo pressure testing and found working.","2020-04-30","","Completed","2020-04-24","No","No","No","External"]
[null,null,null,null,11534,"103_30/4/2020 3:54:50 PM","2020-04-16","Critical Equipment","Ship Staff","Engineering Audit","STEERING GEAR SYSTEM NO 1 HYDRAULIC ALARM ACTIVATION AND AUTO PILOT FAIL ALARM","Navigation - Others","Navigation","Equipment Related","10.1","Medium","","","SYSTEM CHECKS CARRIED OUT AS PER MAKERS AND OFFICE INSTRUCTIONS. SERVICE TECHNICIAN ATTENDED AND RECTIFIED THE FAULT","2020-05-30","","Completed","2020-08-20","No","No","No","Internal","Mr. Kamlesh is looking into this matter Service Engineer has been arranged at Singapore for this."]
[null,null,null,null,10960,"103_31/3/2020 12:59:57 AM","2020-04-16","Defect","Ship Staff","Ship Staff Insp.","#1 MAC damaged","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related","","","","","REPLACED WITH RECEIVED RECONDITIONED SPARE COMPRESSOR","2020-05-30","GILOS - 061 MAIN AIR COMPRESSOR","Completed","2020-07-28","No","No","No","Internal"]
[null,null,null,null,11567,"103_1/5/2020 5:10:19 AM","2020-04-17","Observation","Ship Staff","Ship Staff Insp.","Main hydraulic line for aft main deck hydraulic machinery found holed and leaking\t","Deck - Pipe / Fittings","Mooring","Equipment Related","","","","","The line was removed and fabricated. Fitted back and tested, no leakages observed","2020-04-30","","Completed","2020-04-22","No","No","No","Internal"]
[null,null,null,null,11535,"103_30-Apr-20 8:45:46 PM","2020-04-19","Observation","Ship Staff","Ship Staff Insp.","FOAM MONITOR VALVES AND MOVEMENT FROZEN.","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","FOAM MONITORS MOVED AND GREASING OF FOAM MONITORS AND VALVES CARRIED OUT.","2020-04-30","","Completed","2020-07-04","No","No","No","Internal","Please update if all Foam Monitors valve are free?"]
[null,null,null,null,11550,"103_1/5/2020 6:07:42 AM","2020-04-20","Observation","Ship Staff","Ship Staff Insp.","No grease observed on both hose handling crane and on its wires ","Cargo Mach.,Critical Equip.","General Appearance","Human Error","","","","","Thourough greasing of both hose handling cranes and its wires carried out. All sheaves made free.","2020-07-19","","Completed","2020-05-06","No","No","No","Internal"]
[null,null,null,null,11569,"103_1/5/2020 6:13:16 AM","2020-04-20","Critical Equipment,Observation","Ship Staff","Ship Staff Insp.","Both the accommodation ladders found with no grease.\t","Deck - Pipe / Fittings","Safety / LSA / FFA","Human Error,Inappropriate Procedure","","","","","Thourough greasing of both the accommodation ladders carried out and sheaves made free t rotate.","2020-07-19","","Completed","2020-04-30","No","No","No","Internal"]
[null,null,null,null,10941,"103_30/3/2020 11:14:08 PM","2020-04-20","Defect","Ship Staff","Ship Staff Insp.","ME HFO FLOW METER NOT WORKING.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","ME HFO FLOW METER  REPLACED WITH SPARE AND TESTED WORKING SATISFACTORY","2020-05-30","GILO200029 M/E FLOW METER","Completed","2020-06-20","No","No","No","Internal","27-May-2020: Please proceed and supply vessel as needed with requisition GILO200029 from Alpha Laval for S$3560.29, equivalent to $2,508.85 USD."]
[null,null,null,null,11544,"103_1/5/2020 5:28:57 AM","2020-04-21","Observation","Ship Staff","Ship Staff Insp.","During ballast tank inspection, 3P WBT main line found holed at the seam location of the main valve flange","Hull & Tanks","Cargo / Ballast Systems","External Factors","","","","","The hole has been plugged by wooden piece and soft patch applied to stop the leakage. Item added in the dry dock job list.","2020-06-30","","Completed","2020-05-30","No","No","No","Internal","Please enter the defect in Refman."]
[null,null,null,null,11541,"103_1/5/2020 5:18:28 AM","2020-04-23","Observation","Ship Staff","Ship Staff Insp.","The vapour manifold valves on P & S side manifold found frozen and drain line found choked. Stencil as per ISGOTT found missing and reducer found not properly painted","Deck - Pipe / Fittings","Cargo / Ballast Systems","Behaviour Based,Human Error","","","","","Vapour manifold painted and stencilled as requird. Valves made free to operate.","2020-05-30","","Completed","2020-05-02","No","No","No","Internal","Please advise if RO is raised for this defect?"]
[null,null,null,null,11542,"103_1/5/2020 5:20:55 AM","2020-04-24","Observation","Ship Staff","Ship Staff Insp.","The spindle wheel for Stbd forward vapour manifold drain valve broke while operating","Deck - Pipe / Fittings","General Appearance","Equipment Related","","","","","Spare wheel received and replaced.","2020-06-30","GILO200040","Completed","2020-06-18","No","No","No","Internal","Please advise if GILO200040 is approved from ship. We are not able to see this RFQ in our system."]
[null,null,null,null,11552,"103_1/5/2020 6:39:21 AM","2020-04-25","Observation","Ship Staff","Ship Staff Insp.","SECURING/LOCKING PIN FOUND MISSING AND NO LASHING WIRE ON CARGO AND BALLAST TANK DOMES. CARGO: 3S,4S,4P,5P. BALLAST: 1S,2P,2S,3P,3S,4P,4S ","Deck - Pipe / Fittings","Cargo / Ballast Systems","Human Error,Inappropriate Procedure","","","","","ALL SECURING/LOCKING PINS IN PLACE WITH LASHING WIRE.","2020-07-25","","Completed","2020-05-19","No","No","No","Internal"]
[null,null,null,null,11571,"103_1/5/2020 7:25:25 AM","2020-04-26","Observation","Ship Staff","Ship Staff Insp.","DAVIT WIRES FOR STEERING FLAT DAVIT, PUMPROOM DAVIT AND FPK STORE DAVIT FOUND DRY\t\t\t\t","Deck - Machinery","General Appearance","Human Error,Inappropriate Procedure","","","","","GREASING CARRIED OUT ON ALL WIRES AFTER REMOVING OLD DIRT/GREASE.","2020-07-26","","Completed","2020-04-29","No","No","No","Internal"]
[null,null,null,null,11537,"103_30/4/2020 2:08:08 PM","2020-04-30","Defect","Ship Staff","Ship Staff Insp.","REVERSE POWER RELAY FOR NO 2 AUX. ENGINE MALFUNCTIONING","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.3","Medium","","","REVERSE POWER RELAY FOR NO 2 AUX. ENGINE  TESTED TWICE ON 9/5/20 WORKING SATISFACTORY. WEEKLY ROUTINE OF TESING REVERSE POWER RELAY BEING PRACTISED.","2020-05-30","","Completed","2020-05-09","No","No","No","Internal"]
[null,null,null,null,10956,"103_31/3/2020 12:46:35 AM","2020-05-05","Defect","Ship Staff","Ship Staff Insp.","AE Fuel oil filter found damaged.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Replaced filter with the spare received","2020-05-30","GILO200015 - AE FO SPLIT FILTERS","Completed","2020-08-31","No","No","No","Internal","20-June-2020\n\nPlease be advised that Req. Gilo200015 has been approved and is to be supplied by our side."]
[null,null,null,null,11892,"103_15-May-20 8:06:44 PM","2020-05-07","Defect,Observation","Ship Staff","Ship Staff Insp.","Stbd side lifeboat pressurised fire extinguisher found to be in RED ZONE i.e. having low pressure. Spare Fire extinguisher replaced with the defected one. Now vessel is short of one fire extinguisher as per requirement.","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","SPARES RECIEVED","2020-05-20","R.O. No.: GILO200031","Completed","2020-06-16","No","No","No","Internal","we have quotation, awaiting fixing of the discharge port."]
[null,null,null,null,11885,"103_9/5/2020 10:25:11 AM","2020-05-09","Defect","Ship Staff","Engineering Audit","MGPS CONTROL BOX MALFUNCTION","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","11.1","High","","","MGPS CONTROL BOX NEW SPARE RECEIVED. CONTROL BOX REPLACED AND SYSTEM MADE OPERATIONAL","2020-05-31","GILO200035 MGPS CONTROL BOX","Completed","2020-08-17","No","No","No","Internal","02-June-2020:\nPlease be advised that Req. Gilo200035 has been approved and is to be supplied by our side."]
[null,null,null,null,11888,"103_15/5/2020 4:42:13 PM","2020-05-09","Observation","Ship Staff","Ship Staff Insp.","Several valves in Engine room not holding and leaking (FWG, COPT drain, Hydrophore etc)","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Valves replaced with received new valves.","2020-06-15","GILO200010 - ER VALVES AND STORES FOR CHINA","Completed","2020-06-30","No","No","No","Internal","05-June-2020:\n\nDear Mr. Christos,\n\nPlease find attached cost comparison for GILO200010.\n\nThis is required for valves in Engine room, which are not holding. [Leaking (FWG, COPT drain, Hydrophore etc)]"]
[null,null,null,null,10964,"103_31/3/2020 1:11:10 AM","2020-05-10","Defect","Ship Staff","Ship Staff Insp.","Telephone exchange fault. Internal communication is open to only 1 line.","E/R - Main Engine","Communication","Equipment Related","","","","","Checked the exchange, card removed, reinstalled, system rebooted. Fault rectified","2020-05-30","","Completed","2020-05-12","No","No","No","Internal"]
[null,null,null,null,11893,"103_12/5/2020 7:28:33 PM","2020-05-11","Observation","Ship Staff","Ship Staff Insp.","4 SECTIONS OF DECK AIR LINES FOUND WASTED AND LEAKING.\t","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","Human Error,Inappropriate Procedure","","","","","SECTIONS REMOVED FOR RENEWAL. WILL PUT BACK IN PLACE ONCE COMPLETED RENEWAL.","2020-05-20","","Completed","2020-05-18","No","No","No","Internal"]
[null,null,null,null,11894,"103_12/5/2020 7:25:55 PM","2020-05-11","Observation","Ship Staff","Ship Staff Insp.","PV VALVES FOR 4C,3C,1S COTs FOUND LEAKING","Inert Gas","Cargo / Ballast Systems","External Factors","","","","","Completed overhauling of 4C, 3C and 1S COTs PV Valve.","2020-08-11","","Completed","2020-05-15","No","No","No","Internal"]
[null,null,null,null,11895,"103_15/5/2020 4:03:54 PM","2020-05-12","Observation","Ship Staff","Ship Staff Insp.","1 section of VRCS line forward found leaking due to wastage.","Deck - Pipe / Fittings","Cargo / Ballast Systems","External Factors","","","","","Line removed and new line fabricated and put in place. Line tested and no leaks observed","2020-05-16","","Completed","2020-05-14","No","No","No","Internal"]
[null,null,null,null,11896,"103_15/5/2020 4:17:46 PM","2020-05-12","Observation","Ship Staff","Ship Staff Insp.","1 section of hydraulic line for remote control of mooring winches found leaking due to wastage","Deck - Pipe / Fittings","Mooring","External Factors","","","","","Line removed, fabricated new one and put back. no leakages observed.","2020-05-16","","Completed","2020-05-15","No","No","No","Internal"]
[null,null,null,null,11890,"103_15-May-20 7:13:48 PM","2020-05-13","Observation","Ship Staff","Ship Staff Insp.","All Restricted areas to be marked as per ISPS","Accommodation","ISPS Related","Inappropriate Procedure","7.4","Low","","","Stenciling / posters marked as defined in ISPS.","2020-07-20","","Completed","2020-05-21","No","No","No","Internal"]
[null,null,null,null,12116,"103_21/5/2020 1:44:16 PM","2020-05-21","Defect","Ship Staff","Ship Staff Insp.","GENERAL EMERGENCY ALARM ACTIVATION SWITCH IN FIRE STATION NOT OPERATIONAL","LSA / FFA","Emgcy. Systems","Equipment Related","5.27","Medium","","","GENERAL EMERGENCY ALARM ACTIVATION SWITCH REPLACED WITH SPARE AND TESTED WORKING SATISFACTORY","2020-06-16","GILO200050","Completed","2020-06-25","No","No","No","Internal","GILO200050 is approved for supply from Owners side - Dated :02-June-2020)"]
[null,null,null,null,12118,"103_25/5/2020 11:14:16 AM","2020-05-21","Observation","Ship Staff","Ship Staff Insp.","ME Crankshaft deflection dial gauge damaged","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","Spare received","2020-06-15","GILO200054","Completed","2020-08-15","No","No","No","Internal"]
[null,null,null,null,12119,"103_25/5/2020 11:17:38 AM","2020-05-22","Observation","Ship Staff","Ship Staff Insp.","AE Crankshaft deflection dial gauge damaged","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","New spare received","2020-06-15","GILO200055","Completed","2020-08-15","No","No","No","Internal"]
[null,null,null,null,12117,"103_25/5/2020 11:11:07 AM","2020-05-23","Observation","Ship Staff","Ship Staff Insp.","FWG #1 & #2 does not have chemical dosing system of feed water","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Chemical dosing tank and system installed in place","2020-06-30","GILO200053","Completed","2020-06-30","No","No","No","Internal","we are checking with Owners for Supply. we will update as required."]
[null,null,null,null,12120,"103_26/5/2020 1:17:27 PM","2020-05-25","Observation","Ship Staff","Ship Staff Insp.","GALLYE WASTE DISPOSER STOP SWITCH NOT OPERTIONAL ","Elect. Mach. & Equip.","ISM Related","Equipment Related","","","","","Stop switch replaced with spare one, checked -operational..","2020-06-30","GILO200063","Completed","2020-12-15","No","No","No","Internal"]
[null,null,null,null,13231,"103_8/7/2020 7:47:24 AM","2020-06-02","Defect","Ship Staff","Ship Staff Insp.","Turbo charger and engine RPM display( instrument box )  for Aux. engine no 2 not operational","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Turbo charger and engine RPM display for Aux. engine no 2 not operational same dismentaled and NO. 2 MAIN INSTRUMENT BOX REPLACED WITH RECEIVED SPARE","2020-07-30","GILO200075","Completed","2020-08-18","No","No","No","Internal"]
[null,null,null,null,13232,"103_8/7/2020 7:36:15 AM","2020-06-15","Critical Equipment","Ship Staff","Engineering Audit","SOLENOID COIL AND TRANSFORMER FOR OWS ELECTRICAL PANEL MALFUNCTION","Elect. Mach. & Equip.","MARPOL Related","Equipment Related","","","","","SOLENOID COIL AND TRANSFORMER FOR OWS ELECTRICAL PANEL REPLACED WITH NEW SPARE","2020-07-30","GILO200090","Completed","2020-08-22","No","No","No","Internal"]
[null,null,null,null,13233,"103_8/7/2020 7:42:34 AM","2020-06-15","Defect","Ship Staff","Ship Staff Insp.","Soot blower electrical panel transformer","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","Transformer replaced","2020-07-30","GILO200091","Completed","2020-08-27","No","No","No","Internal"]
[null,null,null,null,13234,"103_8/7/2020 4:46:06 PM","2020-06-30","Breakdown","Ship Staff","Ship Staff Insp.","AE #2 LO cooler gasket leak","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Leaking LO cooler gasket replaced with spare gasket onboard and leak rectified. Spare received","2020-07-31","GILO200094","Completed","2020-08-20","No","No","No","Internal"]
[null,null,null,null,13235,"103_8/7/2020 4:42:18 PM","2020-07-02","Breakdown","Ship Staff","Ship Staff Insp.","FWG ejector pump #1 discharge valve cracked.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Valve replaced with new spare","2020-07-31","","Completed","2020-07-13","No","No","No","Internal"]
[null,null,null,null,13830,"103_26/8/2020 8:34:07 PM","2020-07-03","Observation","Ship Staff","Ship Staff Insp.","Ballast Overboard valve BA039 found leaking as water passing through even the valve is in shut position.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","","","","","New Seatring received and renewed for the ballast valve BA039","2020-08-30","","Completed","2020-08-20","No","No","No","Internal"]
[null,null,null,null,13236,"103_8/7/2020 4:49:45 PM","2020-07-04","Defect","Ship Staff","Ship Staff Insp.","#1 Boiler steam stop valve flange gasket leaking","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Steam stop valve leak retified from flange using metaflex gaskets","2020-07-31","","Completed","2020-07-06","No","No","No","Internal"]
[null,null,null,null,13237,"103_8/7/2020 4:53:43 PM","2020-07-04","Defect","Ship Staff","Ship Staff Insp.","Boiler bottom blowdown valve leak","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Both boilers blowdown valves renewed with spare.","2020-07-31","GILO200100","Completed","2020-09-25","No","No","No","Internal"]
[null,null,null,null,13238,"103_8/7/2020 4:57:36 PM","2020-07-04","Defect","Ship Staff","Ship Staff Insp.","Boiler sea water ingress","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","Sea water ingress noticed during regular boiler water testing. Suspected atmospheric condenser pressure tested and tubes flared. Sysytem is under continous observation with water testing presently at 2 hrs interval. No leak observed since atmospheric condensor tubes were flared.","2020-07-31","","Completed","2020-07-10","No","No","No","Internal"]
[null,null,null,null,13239,"103_7/7/2020 1:19:24 PM","2020-07-06","Critical Equipment","Ship Staff","Ship Staff Insp.","LIFEBOAT STBD SIDE ENGINE STARTING MOTOR NOT OPERATIONAL","Critical Equip.,LSA / FFA","Safety / LSA / FFA","Equipment Related","5.2","Very High","","","Stbd lifeboat engine replaced with received reconditioned spare engine","2020-07-30","RO GILO200099 ","Completed","2020-08-08","No","No","No","Internal"]
[null,null,null,null,13784,"103_5/8/2020 1:19:51 PM","2020-07-12","Defect","Ship Staff","Ship Staff Insp.","LEVEL FLOATS FOR E/R CASCADE , HFO SETTLING AND F.W EXPENSION TANKS NOT OPERATIONL","Elect. Mach. & Equip.,Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","Cascade tank & Expansion Tank floats renewed with new spare ones, HFO Settling tank float switch was tested and working satisfactory.","2020-11-23","GILO200102 ,LEVEL FLOATS FOR E/R TANKS","Completed","2020-11-07","No","No","No","Internal"]
[null,null,null,null,13785,"103_5/8/2020 1:25:36 PM","2020-08-03","Critical Equipment","Ship Staff","Ship Staff Insp.","FIXED GAS DETECTION FLOW FAIL ALARM","Critical Equip.","Safety / LSA / FFA","Equipment Related","","","","","sampling pump diaphrgm renwed, tested and found taking suction, no more flow alarm.Received GILO 200115.","2020-08-30","GILO200115 , Gas Detection System for Ballast tanks","Completed","2020-09-26","No","No","No","Internal"]
[null,null,null,null,13786,"103_29/8/2020 6:14:47 AM","2020-08-09","Defect,Non Conformity,Observation","Ship Staff","Ship Staff Insp.","The locking arrangement for IG branch valve for COT Slop Stbd found broken","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.2","Medium","","","Same has been positively locked by chain and padlock. The arrangement needs to be fabricated.","2020-11-08","","Completed","2020-09-27","No","No","No","Internal"]
[null,null,null,null,13787,"103_29/8/2020 6:19:28 AM","2020-08-09","Observation","Ship Staff","Ship Staff Insp.","The discharge valve of No.1 COP Aus system does not open in manual mode.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","All pneumatic lines inspected, pump room side ann supplies to Positioner and Auto valves checked.In CCR valve D-13 after Auto Manual sector found malfunctionng, smae tempararily made operational.Valve working in manual","2020-11-08","","Completed","2020-10-22","No","No","No","Internal"]
[null,null,null,null,13788,"103_29/8/2020 6:22:12 AM","2020-08-09","Observation","Ship Staff","Ship Staff Insp.","The separator level indication in No.3 COP Aus system does not work properly. The level on the gauge shows empty whereas the separtor is full.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","Fine adjustment on the level transmittor done and now separator level is showing actual level which is empty level and seperator indicator showing zero.","2020-11-08","","Completed","2020-11-05","No","No","No","Internal"]
[null,null,null,null,13789,"103_28/8/2020 7:46:13 AM","2020-08-10","Observation","Ship Staff","Ship Staff Insp.","Mooring winch M1 found very slow in operation. ","Deck - Mooring Machinery","Mooring","Equipment Related","9.14","Medium","","","M1 is now working fine. Hydraulic filters were cleaned and air pressure from regulator adjusted.","2020-11-10","","Completed","2020-11-20","No","No","No","Internal"]
[null,null,null,null,13792,"103_28/8/2020 6:06:11 AM","2020-08-17","Observation","Ship Staff","Ship Staff Insp.","Ballast valves BA028 and BA026 suspected leaking as water flowing through even in shut position.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.15","High","","","Valves to be removed and inspected for leakages","2020-11-17","","Completed","2020-11-24","No","No","No","Internal","BA040 and BA039 made operational and consequently this trouble is sorted out"]
[null,null,null,null,13824,"103_30/8/2020 10:25:25 PM","2020-08-20","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Economiser lagging not in good condition.","Miscellaneous","Eng. / Strg. Comp.","Inappropriate Procedure","","","","","Renewed lagging.","2020-08-31","","Completed","2020-08-28","No","No","No","Internal"]
[null,null,null,null,13825,"103_30/8/2020 10:32:10 PM","2020-08-20","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Confirm soot blower transformer recieved.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","Transformer fitted with the one removed from OWS.","2020-08-30","","Completed","2020-08-29","No","No","No","Internal"]
[null,null,null,null,13826,"103_30/8/2020 10:35:28 PM","2020-08-20","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","EGB Manhole area dirty and soot deposit.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","Manhole area soot deposit cleaned and painted.","2020-08-31","","Completed","2020-08-31","No","No","No","Internal"]
[null,null,null,null,13827,"103_30/8/2020 10:38:27 PM","2020-08-20","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Water leak near stbd side boiler ","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Leak rectified","2020-08-31","","Completed","2020-08-24","No","No","No","Internal"]
[null,null,null,null,13828,"103_30/8/2020 10:47:08 PM","2020-08-20","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","SWL Mark on eye pad emergency escape.","Miscellaneous","Eng. / Strg. Comp.","Inappropriate Procedure","","","","","SWL Stenciled","2020-08-31","","Completed","2020-08-23","No","No","No","Internal"]
[null,null,null,null,13829,"103_30/8/2020 10:50:45 PM","2020-08-20","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Emergency fire p/p trey having water.","E/R - Pumps","Emgcy. Systems","Equipment Related","","","","","Leaking from vaccum pump connection tube. Connection renewed and leak rectified","2020-08-31","","Completed","2020-08-30","No","No","No","Internal"]
[null,null,null,null,13831,"103_30/8/2020 10:54:47 PM","2020-08-20","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Steering panel kept open","Elect. Mach. & Equip.","General Appearance","Equipment Related","","","","","Technician were working on the Steering gear. After completion of work by technician panel closed.","2020-08-20","","Completed","2020-08-20","No","No","No","Internal"]
[null,null,null,null,13832,"103_30/8/2020 10:58:52 PM","2020-08-20","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Rust mark on 7K relief v/v.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Relief valve cleaned and painted.","2020-08-31","","Completed","2020-08-22","No","No","No","Internal"]
[null,null,null,null,13833,"103_30/8/2020 11:03:48 PM","2020-08-20","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Aux Boiler Burner platform is dirty with soot deposit on both burner","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","Both boiler soot deposit cleaned","2020-08-31","","Completed","2020-08-30","No","No","No","Internal"]
[null,null,null,null,13834,"103_30/8/2020 11:07:47 PM","2020-08-20","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Aux Boiler steam drum dirty.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","Aux boiler staem drum top cleaned of dirt.","2020-08-31","","Completed","2020-08-31","No","No","No","Internal"]
[null,null,null,null,13835,"103_30/8/2020 11:15:38 PM","2020-08-20","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Atomising steam v/v lagging bad condition","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Renewed lagging","2020-08-31","","Completed","2020-08-26","No","No","No","Internal"]
[null,null,null,null,13836,"103_30/8/2020 11:23:34 PM","2020-08-20","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Communication fault in Aux eng OMD.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","Communication fault rectified by changing the address of the detector in sequence as required","2020-08-31","","Completed","2020-08-24","No","No","No","Internal"]
[null,null,null,null,13837,"103_30/8/2020 11:27:29 PM","2020-08-20","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Aux Eng tray to clean and lub oil depost to wipe.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","Tray cleaned and mopped","2020-08-31","","Completed","2020-08-24","No","No","No","Internal"]
[null,null,null,null,13838,"103_30/8/2020 11:34:21 PM","2020-08-20","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ME TC Exhaust and inlet pipe paint peel off mark. Exhaust manifold lagging cover (forward end) wasted.  ","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","MT TC exhaust and inlet pipe paint peel off repainted. Lagging on manifold taken out and wasted portion changed","2020-08-31","","Completed","2020-08-31","No","No","No","Internal"]
[null,null,null,null,13839,"103_30/8/2020 10:12:03 PM","2020-08-20","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","CFW Expansion Tank has water and soot mark.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","Cleaned and painted.","2020-08-31","","Completed","2020-08-29","No","No","No","Internal"]
[null,null,null,null,13840,"103_30/8/2020 11:38:55 PM","2020-08-20","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ME fuel p/p leak mark & Cyl head iol leak mark .","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","To be cleaned","2020-08-22","","Completed","2020-08-22","No","No","No","Internal"]
[null,null,null,null,13841,"103_30/8/2020 11:42:44 PM","2020-08-20","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ME Aux blower painting and tank top mopping.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","To be painted and mopped.","2020-08-22","","Completed","2020-08-22","No","No","No","Internal"]
[null,null,null,null,13793,"103_25/8/2020 7:44:17 AM","2020-08-20","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Paint peeled off on few pumproom decks i.w.o the deck opening for personnel rescue","Miscellaneous","General Appearance","Human Error","","","","","Pumproom general cleaning  carried out, Areas  wire brushed and painted.","2020-09-20","","Completed","2020-09-25","No","No","No","Internal"]
[null,null,null,null,13794,"103_25/8/2020 7:48:42 AM","2020-08-20","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Bunker tank Save-all trays to be blasted and painted to avoid wastage of the deck plating.","Deck - Pipe / Fittings","General Appearance","External Factors","","","","","Hydroblasting of bunkar savealls done and painted , some plate wastage has been rectified by soft patch.","2020-11-15","","Completed","2020-11-05","No","No","No","Internal"]
[null,null,null,null,13797,"103_25/8/2020 7:54:38 AM","2020-08-20","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Cap for the Manifold drain line is in poor condition as the threads are worn out.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Human Error","","","","","Cap thread was fabricated and put back.","2020-09-20","","Completed","2020-09-24","No","No","No","Internal"]
[null,null,null,null,13798,"103_25/8/2020 7:56:19 AM","2020-08-20","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Helicopter landing area anti-skid paint to be improved.","Deck - Pipe / Fittings","General Appearance","Human Error","","","","","Derusting of helicopter landing area done by jet chissel. Spot anti skid applied. To hydroblast full area and apply full anti skid.","2020-09-20","","Completed","2020-11-30","No","No","No","Internal","Completed"]
[null,null,null,null,13799,"103_25/8/2020 7:58:57 AM","2020-08-20","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Stbd hose handling crane hook, safety latch noted missing.","Deck - Machinery","Safety / LSA / FFA","Human Error","","","","","Safety latch fabricated and fitted.","2020-09-20","","Completed","2020-09-15","No","No","No","Internal"]
[null,null,null,null,13800,"103_25/8/2020 8:00:19 AM","2020-08-20","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Swimming pool drain valve noted missing from location. ","Deck - Pipe / Fittings","General Appearance","Human Error","","","","","Drain valve in place and working.","2020-09-20","","Completed","2020-10-15","No","No","No","Internal"]
[null,null,null,null,13801,"103_26/8/2020 8:24:44 PM","2020-08-20","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Few light shades in the  pumproom are cracked.","Elect. Mach. & Equip.","Safety / LSA / FFA","Human Error","","","","","Shades were replaced.","2020-09-20","","Completed","2020-09-24","No","No","No","Internal"]
[null,null,null,null,13802,"103_26/8/2020 8:29:04 PM","2020-08-20","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Some of the light shades in the pumproom noted to have missing tube lights.","Elect. Mach. & Equip.","Safety / LSA / FFA","Inappropriate Procedure","","","","","Light shades in pmproom renewed and lights renewed.","2020-09-20","","Completed","2020-09-27","No","No","No","Internal"]
[null,null,null,null,13803,"103_26/8/2020 8:36:34 PM","2020-08-20","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Striking direction arrow stencilled missing on the bitter end for both anchor chains.","Deck - Mooring Machinery","General Appearance","External Factors","","","","","Striking direction arrow has been stencilled on the bitter end .","2020-09-20","","Completed","2020-11-03","No","No","No","Internal"]
[null,null,null,null,13804,"103_26/8/2020 8:40:41 PM","2020-08-20","Critical Equipment,Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","WBT Gas detection system noted in operational.","Hull & Tanks","Cargo / Ballast Systems","Equipment Related","","","","","Fixed gas detection system is operational now. Changed diaform for sampling pump , blow through of sampling lines done . ","2020-11-20","","Completed","2020-09-25","No","No","No","Internal"]
[null,null,null,null,13805,"103_28-Aug-20 2:13:36 AM","2020-08-20","Critical Equipment","Ship Staff","Ship Staff Insp.","N2 Catridge for Galley Fixed Wet chemical Extinguishing system found Expired. ","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","N2 Cartridge renewed.","2020-09-26","GILO200132","Completed","2020-11-20","No","No","No","Internal"]
[null,null,null,null,13807,"103_29/8/2020 8:00:42 AM","2020-08-20","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Mooring roller fairleads, pedestal fairleads and dead man rollers found frozen for forward mooring station","Deck - Mooring Machinery","Mooring","External Factors","9.18","Low","","","Mooring roller was removed , found solid rust inside , same chipped and painted. Now moving free.","2020-09-20","","Completed","2020-10-18","No","No","No","Internal"]
[null,null,null,null,13808,"103_30/8/2020 9:48:05 PM","2020-08-20","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","#1 AHU Leak test carried out, leak found out on the AC compressor unloader","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","Leak rectified and pressure tested. Nitrogen released from the system and system vaccum test completed. Freon gas charging in progress to run the system","2020-09-20","","Completed","2020-09-03","No","No","No","Internal"]
[null,null,null,null,13811,"103_30/8/2020 10:07:08 PM","2020-08-20","Critical Equipment","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Fire Alarm System not all sensor and MCP are working correctly.","Critical Equip.,LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","MCP for pump room entrance changed with new spares , system connected and tested.No fault on the system.Fire detectors tested and alarm sytem working normal","2020-10-15","","Completed","2020-10-23","No","No","No","Internal"]
[null,null,null,null,13812,"103_26/8/2020 8:38:38 PM","2020-08-20","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Radiation hazard marking missing around the FBB and VSAT antenna.","Accommodation","General Appearance","Human Error","","","","","Radiation hazard marking has been stencilled around the FBB and VSAT antenna with a suitable warning notice.","2020-09-20","","Completed","2020-11-02","No","No","No","Internal"]
[null,null,null,null,13814,"103_30/8/2020 11:12:21 PM","2020-08-20","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Atomising steam v/v leaking.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Leaky gasket renewed with new spare.","2020-09-15","","Completed","2020-09-15","No","No","No","Internal"]
[null,null,null,null,13815,"103_30/8/2020 11:19:32 PM","2020-08-20","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","#1 Aux boiler fuel p/p leaking from mechanical seal","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","","","","","Requisition raised for new seal.","2020-09-15","GILO200126 - AUX BOILER F.O. SUPPLY PUMP NO. 1","Completed","2020-11-24","No","No","No","Internal","New Seal Supp;ied, fitted and tried out."]
[null,null,null,null,13816,"103_30/8/2020 11:45:36 PM","2020-08-20","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ER vent fan trunking dust deposit","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","Cleaned and painted wherever required.","2020-09-15","","Completed","2020-09-08","No","No","No","Internal"]
[null,null,null,null,13822,"103_30/8/2020 10:16:44 PM","2020-08-20","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Dosing chemical kept near expansion tank","Miscellaneous","Eng. / Strg. Comp.","Inappropriate Procedure","","","","","Shifted to chemical locker.","2020-08-31","","Completed","2020-08-21","No","No","No","Internal"]
[null,null,null,null,13823,"103_30/8/2020 10:21:36 PM","2020-08-20","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","MAC  supplied (2ND hand) not painted. ","Miscellaneous","Eng. / Strg. Comp.","Inappropriate Procedure","","","","","Painted to machinery green","2020-08-31","","Completed","2020-08-27","No","No","No","Internal"]
[null,null,null,null,null,"103_30/8/2020 9:55:41 PM","2020-08-20","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Galley AC Evaporator coil found wasted beyond repair.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related",null,null,"Not Applicable","Not Applicable","New evaporator has been installed and the system is put back in use. Leak test carried out. All found satisfactory.","2021-02-28","GILO200204","Completed","2021-04-03","No",null,null,"Internal"]
[null,null,null,null,null,"103_25/8/2020 7:50:54 AM","2020-08-20","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Port side Accommodation ladder In/Out control lever noted to be jammed.","Deck - Pipe / Fittings","Safety / LSA / FFA","Equipment Related",null,null,"Not Applicable","Not Applicable","A new control block put in place and tried out, all in order.","2021-02-20",null,"Completed","2021-05-23","No",null,null,"Internal"]
[null,null,null,null,13818,"103_28-Aug-20 2:06:50 AM","2020-08-22","Defect","Ship Staff","Ship Staff Insp.","Foam Monitor found leaking.","LSA / FFA","Safety / LSA / FFA","Equipment Related","12.15","High","","","Foam monitors overhauled and changed bearing and o ring. Now none leaking.","2020-09-10","","Completed","2020-10-16","No","No","No","Internal"]
[null,null,null,null,13813,"103_30/8/2020 10:42:41 PM","2020-08-24","Defect","Ship Staff","Suptd. Insp.","#1 FWG ejector pump motor burnt","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","New spare ejector pump motor installed.","2020-09-15","GILO200131 - FW GENERATOR SW EJECTOR MOTOR NO. 1","Completed","2020-09-09","No","No","No","Internal"]
[null,null,null,null,13810,"103_30/8/2020 10:00:02 PM","2020-08-27","Defect","Ship Staff","Ship Staff Insp.","#2 HFO purifier vertical shaft and bearing damage due to sludge accumulation in the bowl","E/R - Purifier","Eng. / Strg. Comp.","Equipment Related","","","","","Spares received at Port Elizabeth for Vertical shaft.Bowl landed at Port Elizabeth- for reconditioning","2020-11-25","GILO200133 - HFO PURIFIER NO. 2","Completed","2021-01-11","No","No","No","Internal","Spares are received at  Singapore on 27-Dec-2020, same fitted and tried out.\nFound Satisfactory."]
[null,null,null,null,13819,"103_29-Aug-20 12:46:44 AM","2020-08-28","Defect","Ship Staff","Ship Staff Insp.","Anemometer True wind direction and speed not available as no GPS input to anemometer.Only relative wind and speed displayed.","Navigation - Others","Navigation","Equipment Related","","","","","Option of giving NMEA signal to the Anemometer is not available with this unit.","2020-09-28","","Completed","2020-10-21","No","No","No","Internal"]
[null,null,null,null,13820,"103_29-Aug-20 12:55:30 AM","2020-08-28","Other","Ship Staff","Ship Staff Insp.","VDR - Alarm on VDR display panel for Anemometer. Missing data from Anemometer.","Navigation - VDR / BNWAS","Navigation","Equipment Related","","","","","VDR has no alarm. ","2020-09-28","","Completed","2020-10-14","No","No","No","Internal"]
[null,null,null,null,13821,"103_29/8/2020 6:27:41 AM","2020-08-28","Observation","Ship Staff","Ship Staff Insp.","The ballast valve BA039 found not holding as the water is flowing pass thrpugh the valve even in shut condition","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.21","High","","","Valve replaced with new one.","2020-11-27","","Completed","2020-11-30","No","No","No","Internal"]
[null,null,null,null,16271,"103_12/10/2020 4:38:41 AM","2020-09-07","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Ships Name on Port & stbd side is very small.Owner observation.","Hull & Tanks","General Appearance","External Factors","","","","","To put new Name Markings","2020-11-27","","Completed","2020-11-29","No","No","No","Internal",""]
[null,null,null,null,16272,"103_12/10/2020 5:07:04 AM","2020-09-07","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Several accomodation windows on upper deck found rust signs","Accommodation","General Appearance","External Factors","","","","","clean and derust and paint","2020-10-25","","Completed","2020-11-30","No","No","No","Internal"]
[null,null,null,null,16279,"103_12/10/2020 1:31:49 AM","2020-09-07","Defect,Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Aux engine L.O cooler (Plate Cooler)slight oil leaks plate edges","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","End Plate retightened equally and leaks rectified.","2020-09-20","","Completed","2020-09-20","No","No","No","Internal"]
[null,null,null,null,16289,"103_12/10/2020 4:23:13 AM","2020-09-07","Defect,Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","VRCS Room -Pump station -oil leaks noted in save all","Deck - Machinery","Cargo / Ballast Systems","Equipment Related","","","","","Noted oil level in tank excessive and oil coming out from breather, oil level lowered to Normal level.","2020-09-20","","Completed","2020-09-22","No","No","No","Internal"]
[null,null,null,null,16290,"103_12/10/2020 5:15:56 AM","2020-09-07","Defect,Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Elevator \"A\" Deck Push button secured with tape","Accommodation","Eng. / Strg. Comp.","Equipment Related","","","","","NOW lift stops at A deck and puch button works fine also on A deck.","2020-10-15","","Completed","2020-10-12","No","No","No","Internal"]
[null,null,null,null,16292,"103_12/10/2020 4:49:54 AM","2020-09-07","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","MCSW Pump coupling cover damaged","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","","","","","New cover was fabricated and fixed","2020-10-16","","Completed","2020-10-28","No","No","No","Internal"]
[null,null,null,null,16294,"103_11/10/2020 11:50:09 AM","2020-09-07","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Bridge watch unit for engine room watch changeover found to be out of order.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","Replaced the same with newly received spare. No w working satisfactory.","2020-11-30","GILO200148","Completed","2020-11-25","No","No","No","Internal"]
[null,null,null,null,16295,"103_12/10/2020 4:46:12 AM","2020-09-07","Defect,Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Hand rails on funnel deck damaged","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Cold repairs carried out. ","2020-10-24","","Completed","2020-11-07","No","No","No","Internal"]
[null,null,null,null,16297,"103_12/10/2020 4:58:44 AM","2020-09-07","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ME Exhaust Pipe leak on B-Deck(Above Incinerator Platform)","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Insulation was removed and bellow was inspected. No leaks observed. ","2020-11-25","","Completed","2020-11-06","No","No","No","Internal"]
[null,null,null,null,16298,"103_12/10/2020 4:43:25 AM","2020-09-07","Defect,Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ME Funnel Exh gas outlet screen on Funnel deck damaged","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Exhaust funnel screeen secured with new angle bar, and screen mesh repaired-additional piece added.","2020-10-24","","Completed","2020-12-01","No","No","No","Internal"]
[null,null,null,null,16299,"103_12/10/2020 4:54:10 AM","2020-09-07","Defect,Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Aux engine No.3 TC L.O Pressure Guage discoloured","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Pressure guage renewed.","2020-11-05","GILO200166","Completed","2020-11-20","No","No","No","Internal"]
[null,null,null,null,16278,"103_9/10/2020 4:57:59 PM","2020-09-08","Critical Equipment","Ship Staff","Ship Staff Insp.","The Oil mist detector is showing communication fault. ","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.21","Medium","","","Interface PCB Received, fittted and tested for Main engine .Working satisfactory","2020-09-30","GILO200141","Completed","2020-10-05","No","No","No","Internal"]
[null,null,null,null,16288,"103_12/10/2020 1:23:41 AM","2020-09-10","Critical Equipment","Ship Staff","Ship Staff Insp.","Emergency fIR PUMP TAKING LONG TIME TO TAKE SUCTION(Ballast condition)","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.41","Very High","","","Priming device overhauled, seals renewed.Suction filter cleaned and NR valve inspectred.","2020-09-14","","Completed","2020-09-14","No","No","No","Internal"]
[null,null,null,null,16282,"103_12/10/2020 1:51:54 AM","2020-09-15","Critical Equipment","Ship Staff","Ship Staff Insp.","Starboard Life boat engine starting diffculty, and not going Astern ahead.Engine unable to go full throtle on Astern directions","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.29","High","","","The fuel cable connection on the lifebaot engine made free, made free,operated severl time in idle mode.Ahead-Astrern Cable securing arrangent not proper and getting resistance to move, same removed, readjusted and alaigned.Tried-working satisfactory.","2020-09-15","","Completed","2020-09-16","No","No","No","Internal"]
[null,null,null,null,16291,"103_12/10/2020 2:17:07 AM","2020-09-15","Defect","Ship Staff","Ship Staff Insp.","Sludge transfer pipe arrangement from shore connection -intermediate pipe section to deck slop tank -leaking at several places","Deck - Pipe / Fittings","MARPOL Related","Equipment Related","","","","","Leaky pipe sections renewed.","2020-10-30","","Completed","2020-10-14","No","No","No","Internal"]
[null,null,null,null,16285,"103_12/10/2020 2:09:53 AM","2020-09-16","Critical Equipment","Ship Staff","Ship Staff Insp.","Main engine fuel leakage alarm not working","E/R - Main Engine,Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","Float chamber isolated and leak chamber drained, flaot removed and checked out side, redo all electrical connections, tried out, working satisfactory.","2020-09-18","","Completed","2020-09-17","No","No","No","Internal"]
[null,null,null,null,16286,"103_12/10/2020 2:20:53 AM","2020-09-16","Defect","Ship Staff","Suptd. Insp.","FWG 2 production is less","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Evaporator chemical cleaning carried out, Demister cleaned and conbenser cleaned.Flow meter pipe checked.Production improved .","2020-10-04","","Completed","2020-10-08","No","No","No","Internal"]
[null,null,null,null,16284,"103_12/10/2020 2:03:09 AM","2020-09-20","Observation","Ship Staff","Ship Staff Insp.","Sewage treatment plant Recirculation pipe not clear.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","All stages chanbers flushed,  recirculation pipes cleaned and flow clearly visible","2020-09-21","","Completed","2020-10-22","No","No","No","Internal"]
[null,null,null,null,16287,"103_12/10/2020 2:33:27 AM","2020-09-23","Defect","Ship Staff","Ship Staff Insp.","Vaccum toilet system in operational as vacuum not buiding.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Ejector nozzle section removed, was choked , same cleared, nozzle renewed.System checked for vacuum, put in service, working satisfactory","2020-09-24","","Completed","2020-09-24","No","No","No","Internal"]
[null,null,null,null,16296,"103_12/10/2020 2:28:38 AM","2020-09-25","Defect,Observation","Ship Staff","Ship Staff Insp.","Aux boilers upon change over to MGO , did not show change over on the Saacke Panel & LSMGO pump not starting in Auto on Auto mode operation.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.9","Medium","","","To seek makers advice.Trouble shoot/study/investigation in progress.Update on All microswitches were cleanes and de-rusted. Change over valve eased up. Now the change over is showing on Saccke panel and the pump is cutting and cutting off on Auto.","2020-11-15","","Completed","2020-11-06","No","No","No","Internal"]
[null,null,null,null,16283,"103_12/10/2020 1:58:02 AM","2020-09-26","Defect","Ship Staff","Ship Staff Insp.","Aux boiler No.2 Econimiser maint staem valve leaking from bonnet.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","Vlave bonnet gasket renewed.Leak Rectified.","2020-10-28","","Completed","2020-10-27","No","No","No","Internal"]
[null,null,null,null,16280,"103_12/10/2020 1:38:03 AM","2020-09-27","Defect","Ship Staff","Ship Staff Insp.","No.1 Provision Compressor Motor Run hot and tripped on Overlaod","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Motor Insulation checked-Found ok.Contactor found burnt and same replaced with sapre one","2020-09-28","","Completed","2020-09-28","No","No","No","Internal"]
[null,null,null,null,16293,"103_12/10/2020 4:14:57 AM","2020-10-05","Defect","Ship Staff","Ship Staff Insp.","Ballast Line Overboard Valve BA040 (Inside 5PWBT) Actuator defective and valve struck in open position","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","","","","","Received new actuator at Port Elizabeth and same placed on BA040 and tested . Confirm its working both remote hydraulically and manual handwheel.","2020-11-04","","Completed","2020-11-03","No","No","No","Internal"]
[null,null,null,null,16281,"103_12/10/2020 1:43:06 AM","2020-10-07","Observation","Ship Staff","Ship Staff Insp.","A/C compressor No.1 noted fluctuating between stages and not steady,though  suction pressure seems sufficient.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Unloading solenoind power supply checked, the control circuit fuses were replaced,Minutr Adjustments to 2nd & 3rd stages cut in cut out ,Slight Gas charged in system and put on Auto Operation","2020-10-09","","Completed","2020-10-09","No","No","No","Internal"]
[null,null,null,null,16276,"103_16/12/2020 4:42:01 PM","2020-11-18","Defect,Observation","Ship Staff","Ship Staff Insp.","Boiler Blowdown Shipside overbaord valve in bad condition/Corroded","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","Vessel has raised requisition for new valves.Kept under close monitioring.","2020-12-31","GILO200197","Completed","2020-12-27","No","No","No","Internal","Both Valve renewed with assistance of diver"]
[null,null,null,null,16275,"103_15/12/2020 4:46:48 PM","2020-12-07","Defect","Ship Staff","Ship Staff Insp.","Vacuum Condenser outlet pipe section leaking -hole at flange weld","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Temporary cold work carried out from outside,will open up pipe section to do reapirs from inside -during ballast passage.","2020-12-31","","Completed","2021-01-11","No","No","No","Internal","Repair carried out after removing the pipe"]
[null,null,null,null,null,"103_15/5/2020 4:59:21 PM","2020-12-20","Defect","Ship Staff","Ship Staff Insp.","#2 Air Dryer defective","Miscellaneous","Eng. / Strg. Comp.","Equipment Related",null,null,"Not Applicable","Not Applicable","New air dryer installed. Now it's operational.","2021-03-20","GILO200077","Completed","2021-04-13","No",null,null,"Internal"]
[null,null,null,null,16900,"103_Sat Jan 09 2021 08:37:17 GMT+0000","2020-12-26","Observation","Owner / Marine / Tech. Suptd.","Bunkering Audit","Bunker line goose neck valve on deck no notice posted for inadvertent opening or secured / sealed to avoid opening by mistake.","Deck - Pipe / Fittings","MARPOL Related","Human Error","2.16","Medium","","","In order to avoid any accidental opening of the valves a notice has been posted and the valves have been sealed.","2021-01-26","","Completed","2021-01-14","No","No","No","Internal"]
[null,null,null,null,16901,"103_Sat Jan 09 2021 08:38:30 GMT+0000","2020-12-26","Observation","Owner / Marine / Tech. Suptd.","Cargo Audit","Ballast Eductor suction gauge showing incorrect reading.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.51","Low","","","The defective gauge was rectified and compared.","2021-01-26","","Completed","2021-01-15","No","No","No","Internal"]
[null,null,null,null,16902,"103_Sat Jan 09 2021 08:40:01 GMT+0000","2020-12-26","Observation","Owner / Marine / Tech. Suptd.","Cargo Audit","Leak noticed from stripping pump gland.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.15","High","","","The gland packing of the stripping pump was renewed after inspection. ","2021-01-26","","Completed","2021-01-15","No","No","No","Internal"]
[null,null,null,null,16903,"103_Sat Jan 09 2021 08:42:23 GMT+0000","2020-12-26","Observation","Owner / Marine / Tech. Suptd.","Nav Audit / Verification","Anchor watch change over check list not signed for change of watch at 2000 hrs LT on 26 Dec 2020","Documentation,Navigation - Others","Navigation","Behaviour Based","","","","","Briefing of all watch keepers to be carried out to complete the change of watch checklists without fail.","2020-12-28","","Completed","2020-12-28","No","No","No","Internal"]
[null,null,null,null,16904,"103_Sat Jan 09 2021 08:44:14 GMT+0000","2020-12-26","Observation","Owner / Marine / Tech. Suptd.","Nav Audit / Verification","Aldis lamp battery check log not updated.","Navigation - Others","Navigation","Human Error","","","","","Log to be updated each time the battery checks are carried out by the electrical officer.","2020-12-28","","Completed","2020-12-27","No","No","No","Internal"]
[null,null,null,null,17101,"103_Thu Jan 14 2021 07:37:23 GMT+0000","2020-12-27","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Steam coils of Slops tanks to is rusty.","Deck - Pipe / Fittings","General Appearance","External Factors","","","","","Steam coils of Slops tanks de-rusted and painted.","2021-03-26","","Completed","2021-02-01","No","No","No","Internal"]
[null,null,null,null,17102,"103_Thu Jan 14 2021 07:39:25 GMT+0000","2020-12-27","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Windlasses fittings found rusty","Deck - Mooring Machinery","General Appearance","External Factors","9.2","Very High","","","Windlasses fittings de- rusted and painted.","2021-01-26","","Completed","2021-02-23","No","No","No","Internal"]
[null,null,null,null,17103,"103_Thu Jan 14 2021 07:41:24 GMT+0000","2020-12-27","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Mooring rollers in way of aft springs are frozen.","Deck - Machinery,Deck - Mooring Machinery","Mooring","Equipment Related","9.18","Low","","","Mooring rollers in way of aft springs freed and greased.","2021-01-26","","Completed","2021-01-28","No","No","No","Internal"]
[null,null,null,null,17104,"103_Thu Jan 14 2021 07:44:34 GMT+0000","2020-12-27","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","4C PV valve was observed to be leaking.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.4","Medium","","","Vessel has tried to lap the disc; leak has reduced substantially.","2021-01-26","","Completed","2021-02-04","No","No","No","Internal"]
[null,null,null,null,17108,"103_Thu Jan 14 2021 08:12:30 GMT+0000","2020-12-27","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Mushroom vents on sunken deck needs maintenance.","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","Equipment Related","11.1","High","","","Mushroom vents on sunken deck de-rusted and painted.","2021-01-26","","Completed","2021-02-25","No","No","No","Internal"]
[null,null,null,null,17109,"103_Thu Jan 14 2021 08:14:21 GMT+0000","2020-12-27","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Passage between emergency generator room and funnel deck not in order.","Miscellaneous","General Appearance","Behaviour Based","","","","","Passage between emergency generator room and funnel deck cleaned and arranged.","2021-03-26","","Completed","2021-02-27","No","No","No","Internal"]
[null,null,null,null,17110,"103_Thu Jan 14 2021 08:17:28 GMT+0000","2020-12-27","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Stores items are not kept in tidy condition.","Miscellaneous","General Appearance","Behaviour Based","11.3","Medium","","","Housekeeping of the stores arranged.","2021-01-26","","Completed","2021-01-16","No","No","No","Internal"]
[null,null,null,null,17112,"103_Thu Jan 14 2021 09:43:56 GMT+0000","2020-12-27","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Water cooler on C deck non-functional.","Accommodation","MLC Related","Equipment Related","","","","","Water cooler on C deck is now functional.","2021-03-26","","Completed","2021-01-12","No","No","No","Internal"]
[null,null,null,null,17113,"103_Thu Jan 14 2021 09:45:27 GMT+0000","2020-12-27","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Auxiliary boiler atomizing valve steam is leaking","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","Auxiliary boiler atomizing valve steam leak rectified by renewing the gland packing.","2021-01-26","","Completed","2021-01-13","No","No","No","Internal"]
[null,null,null,null,17114,"103_Thu Jan 14 2021 09:48:13 GMT+0000","2020-12-27","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Auxiliary boiler no.2 steam pressure transmitter line is leaking","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","Auxiliary boiler no.2 steam pressure transmitter line leak was rectified by renewing the small pipe section which had the leak.","2021-01-26","","Completed","2021-01-13","No","No","No","Internal"]
[null,null,null,null,17115,"103_Thu Jan 14 2021 09:49:53 GMT+0000","2020-12-27","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Service air bottle cosmetic upgradation to be carried out.","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related","","","","","Service air bottle cosmetic upgradation  carried out.","2021-01-26","","Completed","2021-01-23","No","No","No","Internal"]
[null,null,null,null,17116,"103_Thu Jan 14 2021 09:52:53 GMT+0000","2020-12-27","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Economizer soot blower area cosmetic appearance not good","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","Economizer soot blower area cosmetic upgradation was carried out. Save all tray was also cleaned and painted.","2021-01-26","","Completed","2021-01-17","No","No","No","Internal"]
[null,null,null,null,17117,"103_Thu Jan 14 2021 10:07:14 GMT+0000","2020-12-27","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","DG exhaust manifold high temperature paint peeling off.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","DG exhaust manifold high temperature painting carried out.","2021-01-26","","Completed","2021-01-20","No","No","No","Internal"]
[null,null,null,null,17118,"103_Thu Jan 14 2021 10:08:37 GMT+0000","2020-12-27","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","DG aft area and bulkhead cosmetic appearance not satisfactory","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","DG aft area and bulkhead cosmetic improvement carried out.","2021-01-26","","Completed","2021-01-17","No","No","No","Internal"]
[null,null,null,null,17120,"103_Thu Jan 14 2021 10:11:34 GMT+0000","2020-12-27","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Fresh water generator no.1 has salt deposits.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Fresh water generator no.1 salt deposits cleaned and leaks were rectified. Cosmetic upgradation carried out.","2021-01-26","","Completed","2021-01-07","No","No","No","Internal"]
[null,null,null,null,17121,"103_Thu Jan 14 2021 10:12:49 GMT+0000","2020-12-27","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Lagging on warming up valve for COPT is missing.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Lagging on warming up valve for COPT was installed.","2021-01-26","","Completed","2021-01-15","No","No","No","Internal"]
[null,null,null,null,17123,"103_Thu Jan 14 2021 10:17:14 GMT+0000","2020-12-27","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Newly installed overboard valves for Boiler Blowdown and Galley Drain  to be painted with same as other overboard valve.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Newly installed overboard valves were painted same as other valves.","2021-01-26","","Completed","2021-01-02","No","No","No","Internal"]
[null,null,null,null,17124,"103_Thu Jan 14 2021 10:19:00 GMT+0000","2020-12-27","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Vacuum condenser sea water outlet line has leak, which is temporary repaired.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","The intermediate section was removed and repairs were carried out both from inside and outside. ","2021-01-26","","Completed","2021-01-15","No","No","No","Internal"]
[null,null,null,null,null,"103_Thu Jan 14 2021 10:14:37 GMT+0000","2020-12-27","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","LT cooler no.1 sea water inlet valve actuator broken.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related",10.33,"High","Not Applicable","Not Applicable","Actuator raised and fitted.","2021-01-26","GILO200169","Completed","2021-03-01","No",null,null,"Internal"]
[null,null,null,null,null,"103_Thu Jan 14 2021 09:42:13 GMT+0000","2020-12-27","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Cement coming out of C deck alleyway floor mat.","Accommodation","MLC Related","Equipment Related",11.13,"Low","Not Applicable","Not Applicable","Cement coming out of C deck alleyway floor mat attended. Cement layer broken and fresh layer laid.","2021-03-26",null,"Completed","2021-04-02","No",null,null,"Internal"]
[null,null,null,null,17748,"103_31/1/2021 9:29:04 AM","2021-01-09","Observation","Ship Staff","Ship Staff Insp.","One of the section of deck service air was observed to be pin holed. ","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.4","Very High","","","The holed section was dismantled and taken to engine room work shop where it was cropped and new section was welded. Same was pressure tested and fitted back on the deck after painting.    PMS Job order No V-GILO006881/21.","2021-01-31","","Completed","2021-01-11","No","No","No","Internal"]
[null,null,null,null,null,"103_7/4/2021 7:59:47 AM","2021-03-01","Defect","Ship Staff","Ship Staff Insp.","Fresh water generator no.2 salinity sensor showing negative readings\t","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Sensor was cleaned and installed again. Is now working satisfactory.","2021-07-01","GILO210075","Completed","2021-06-22","No",null,null,"Internal"]
[null,null,null,null,null,"103_26/3/2021 7:49:34 PM","2021-03-26","Defect","Ship Staff","Ship Staff Insp.","Slew Motor control block in Stbd side hose handling crane leaking oil.\t","Deck - Machinery","Cargo / Ballast Systems","Equipment Related",8.5,"Very High","Not Applicable","Not Applicable","Block renewed.","2021-04-30",null,"Completed","2021-04-04","No",null,null,"Internal"]
[null,null,null,null,null,"103_26/3/2021 7:54:58 PM","2021-03-26","Defect","Ship Staff","Ship Staff Insp.","Doppler log is erractic\t","Navigation - Echo Sounder / Speed Log","Navigation","Equipment Related",4.7,"High","Not Applicable","Not Applicable","Doppler log sensor renewed.","2021-04-30",null,"Completed","2021-04-04","No",null,null,"Internal"]
[null,null,null,null,null,"103_26/3/2021 7:56:58 PM","2021-03-26","Defect","Ship Staff","Ship Staff Insp.","Echo sounder not displaying depths when vessel is stopped","Navigation - Echo Sounder / Speed Log","Navigation","Equipment Related",4.7,"High","Not Applicable","Not Applicable","Echo sounder sensor renewed.","2021-04-30",null,"Completed","2021-04-04","No",null,null,"Internal"]
[null,null,null,null,null,"103_26/3/2021 9:00:42 PM","2021-03-26","Defect","Ship Staff","Ship Staff Insp.","Tiles broken/missing from common areas such as pantry/ Galley and Crew Cabins.","Accommodation","General Appearance","Equipment Related",11.13,"Low","Not Applicable","Not Applicable","Broken tiles replaces with the new ones and fixed with white cement.","2021-05-31",null,"Completed","2021-04-30","No",null,null,"Internal"]
[null,null,null,null,null,"103_26/3/2021 7:32:36 PM","2021-03-26","Defect","Ship Staff","Ship Staff Insp.","No driers in Ship Linen Laundry and Officers Laundry","Accommodation","General Appearance","Equipment Related",11.14,"Medium","Not Applicable","Not Applicable","Driers received at Fujariah on 03 April 2021. Same installed in laundries.","2021-04-30",null,"Completed","2021-04-17","No",null,null,"Internal"]
[null,null,null,null,null,"103_26/3/2021 7:34:54 PM","2021-03-26","Defect","Ship Staff","Ship Staff Insp.","Pumproom light covers are cracked and seals are damaged.","Elect. Mach. & Equip.","Safety / LSA / FFA","Equipment Related",8.48,"Medium","Not Applicable","Not Applicable","Spares received at Fujairah on 03 April 2021. Lights  renewed .","2021-04-30",null,"Completed","2021-04-22","No",null,null,"Internal"]
[null,null,null,null,null,"103_26/3/2021 7:47:31 PM","2021-03-26","Defect","Ship Staff","Ship Staff Insp.","Few hoses in hose handling cranes are found with heavily rusted ends. Denso tapes missing from Hose ends","Deck - Machinery","Cargo / Ballast Systems","Equipment Related",8.5,"Very High","Not Applicable","Not Applicable","Rusted hoses renewed and covered with the denso tape at ends.","2021-04-30",null,"Completed","2021-04-04","No",null,null,"Internal"]
[null,null,null,null,null,"103_26/3/2021 8:30:36 PM","2021-03-26","Defect","Ship Staff","Ship Staff Insp.","Many valves on deck found with wasted valve wheels\t","Deck - Pipe / Fittings","General Appearance","Equipment Related",11.4,"Very High","Not Applicable","Not Applicable","Spare wheels received at Fujairah on 03 April 2021. Wasted wheels renewed.","2021-05-31",null,"Completed","2021-04-05","No",null,null,"Internal"]
[null,null,null,null,null,"103_26/3/2021 8:34:41 PM","2021-03-26","Defect","Ship Staff","Ship Staff Insp.","Cargo sampler leaking from seals and spraying oil on deck when used. Vessel has only 1 cargo sampler","Cargo Mach.","Cargo / Ballast Systems","Equipment Related",8.16,"Very High","Not Applicable","Not Applicable","New seal received and fit in place.","2021-04-30",null,"Completed","2021-04-22","No",null,null,"Internal"]
[null,null,null,null,null,"103_26/3/2021 8:59:08 PM","2021-03-26","Defect","Ship Staff","Ship Staff Insp.","Crew Pantry Water Boiler leaking from Valve","Accommodation","General Appearance","Equipment Related",11.13,"Low","Not Applicable","Not Applicable","A new electric water boiler put in place once recevied in Fujairah on 03 Apr 2021.","2021-04-30",null,"Completed","2021-04-04","No",null,null,"Internal"]
[null,null,null,null,null,"103_26/3/2021 9:50:33 PM","2021-03-26","Defect","Ship Staff","Ship Staff Insp.","Drinking water sterlizer not operational due to defective lamp ballast.\t","Accommodation","General Appearance","Equipment Related",11.13,"Low","Not Applicable","Not Applicable","Sterlizer ballast was renewed, UV lamp renewed along with the sleeve.","2021-04-30",null,"Completed","2021-04-20","No",null,null,"Internal"]
[null,null,null,null,null,"103_26/3/2021 9:18:55 PM","2021-03-26","Defect","Ship Staff","Ship Staff Insp.","Water stoppage in Accommodation and toilet when Engine room hot well is being filled up as the hot well filling line is also from the Fresh Water hydrophore.","Accommodation","General Appearance","Equipment Related",11.13,"Low","Not Applicable","Not Applicable","New pipe line fabricated and fitted to segregate the Hot well filling line from Fresh Water hydrophore.","2021-05-31",null,"Completed","2021-04-15","No",null,null,"Internal"]
[null,null,null,null,null,"103_26/3/2021 7:20:57 PM","2021-03-26","Defect","Ship Staff","Ship Staff Insp.","Two Foam Monitors leaking from bearings.","LSA / FFA","Safety / LSA / FFA","Equipment Related",5.35,"Medium","Not Applicable","Not Applicable","Spares received at Fujariah on 03 April 2021. Orings renewed.","2021-04-30",null,"Completed","2021-04-15","No",null,null,"Internal"]
[null,null,null,null,null,"103_26/3/2021 9:13:55 PM","2021-03-26","Defect","Ship Staff","Ship Staff Insp.","No 1 Aircon system is not operational.","Accommodation","General Appearance","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Spare bypass valve received and same was fixed. Compressor is now working satisfactorily.","2021-05-31",null,"Completed","2021-05-13","No",null,null,"Internal"]
[null,null,null,null,null,"103_26/3/2021 8:24:36 PM","2021-03-26","Defect","Ship Staff","Ship Staff Insp.","4 COW Pipeline root valves not holding\t","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related",8.34,"High","Not Applicable","Not Applicable","Defective valves replaced with the new ones. ","2021-04-30",null,"Completed","2021-05-16","No",null,null,"Internal"]
[null,null,null,null,null,"103_2/4/2021 12:40:58 AM","2021-03-26","Defect","Ship Staff","Ship Staff Insp.","Aft STS Mooring Capston inoperational.\t","Deck - Mooring Machinery","Mooring","Equipment Related",9.16,"High","Not Applicable","Not Applicable","Aft STS Mooring is now working. One of the fuse was renewed. ","2021-05-31",null,"Completed","2021-05-25","No",null,null,"Internal"]
[null,null,null,null,null,"103_26/3/2021 8:21:31 PM","2021-03-26","Defect","Ship Staff","Ship Staff Insp.","Power sockets for Day Light Signaling lamp ( Aldis lamp) in bridge front and bridge wings not working.","Navigation - Others","Navigation","Equipment Related",4.7,"High","Not Applicable","Not Applicable","Found one of the fuse not working. Same was renewed. Now the power sockets are working.","2021-04-30",null,"Completed","2021-05-16","No",null,null,"Internal"]
[null,null,null,null,null,"103_26/3/2021 9:27:12 PM","2021-03-26","Defect","Ship Staff","Ship Staff Insp.","Bridge duct heaters for Bridge windows not operational","Navigation - Others","Navigation","Equipment Related",4.7,"High","Not Applicable","Not Applicable","Duct heater working. ","2021-04-30",null,"Completed","2021-05-25","No",null,null,"Internal"]
[null,null,null,null,null,"103_26/3/2021 8:54:29 PM","2021-03-26","Defect","Ship Staff","Ship Staff Insp.","CCR VHF stopped reception for 1 day during the last discharging at Thanh Hoa, Vietnam. After 1 day of inoperation, VHF started reception.\t","Miscellaneous","Communication","Equipment Related",4.2300000000000004,"High","Not Applicable","Not Applicable","Rectified. ","2021-06-30",null,"Completed","2021-06-17","No",null,null,"Internal"]
[null,null,null,null,null,"103_26/3/2021 7:40:16 PM","2021-03-26","Defect","Ship Staff","Ship Staff Insp.","Stbd side Hose handling crane mast inspection cover wasted in the edges","Deck - Machinery","Cargo / Ballast Systems","Equipment Related",8.5,"Very High","Not Applicable","Not Applicable","Wasted sections cropped and renewed with inserts.","2021-05-31",null,"Completed","2021-06-22","No",null,null,"Internal"]
[null,null,null,null,null,"103_26/3/2021 8:36:40 PM","2021-03-26","Defect","Ship Staff","Ship Staff Insp.","Deck Seal overboard vertical pipeline in Pumproom is having a soft patch.","Inert Gas","Cargo / Ballast Systems","Equipment Related",8.27,"Medium","Not Applicable","Not Applicable","The holed section of the pipe renewd.","2021-04-30",null,"Completed","2021-06-06","No",null,null,"Internal"]
[null,null,null,null,null,"103_26/3/2021 8:15:06 PM","2021-03-26","Defect","Ship Staff","Ship Staff Insp.","Slop Tank COW Machines not working.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related",8.34,"High","Not Applicable","Not Applicable","Slop Tank COW Machines overhauled and madeoperational.","2021-07-31",null,"Completed","2021-06-07","No",null,null,"Internal"]
[null,null,null,null,null,"103_26/3/2021 8:57:18 PM","2021-03-26","Defect","Ship Staff","Ship Staff Insp.","Water overflowing into crew pantry from the diswasher drain pipe.\t","Accommodation","General Appearance","Equipment Related",11.13,"Low","Not Applicable","Not Applicable","Scupper drain line cleared.","2021-07-30",null,"Completed","2021-06-10","No",null,null,"Internal"]
[null,null,null,null,null,"103_2/4/2021 8:29:59 AM","2021-03-27","Observation","Ship Staff","Ship Staff Insp.","Sludge pump bearing condition is not good\t","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Sludge pump bearings were renewed.","2021-05-01","GILO210051","Completed","2021-04-18","No",null,null,"Internal"]
[null,null,null,null,null,"103_1/4/2021 11:43:31 AM","2021-03-27","Defect","Ship Staff","Ship Staff Insp.","Economizer feed pump leaking from forward mechanical seal","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Forward seal leak rectified.","2021-06-08",null,"Completed","2021-06-23","No",null,null,"Internal"]
[null,null,null,null,null,"103_2/4/2021 8:27:15 AM","2021-03-27","Observation","Ship Staff","Ship Staff Insp.","Auxilary boiler dosing line is choked.\t\t","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Choked sections cleared.","2021-07-01",null,"Completed","2021-06-23","No",null,null,"Internal"]
[null,null,null,null,null,"103_2/4/2021 8:25:32 AM","2021-03-28","Observation","Ship Staff","Ship Staff Insp.","Main engine and Generator auto-backwash filter chang-over valve leaking\t","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Change over section cleaned and put back. No leaks observed.","2021-05-01",null,"Completed","2021-06-10","No",null,null,"Internal"]
[null,null,null,null,null,"103_7/4/2021 8:02:27 AM","2021-03-29","Defect","Ship Staff","Ship Staff Insp.","AE #2 priming LO pump motor burnt","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","New motor received and was replaced.","2021-05-01","GILO210061","Completed","2021-04-22","No",null,null,"Internal"]
[null,null,null,null,null,"103_10/4/2021 8:45:38 AM","2021-03-31","Defect","Ship Staff","Ship Staff Insp.","Boiler water circulating pump no.2 making abnormal sound. ","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Pump overhauled. Job order no.                          V-GILO000664/20\t","2021-04-20",null,"Completed","2021-04-10","No",null,null,"Internal"]
[null,null,null,null,null,"103_12/4/2021 2:52:34 PM","2021-04-12","Defect","Ship Staff","Ship Staff Insp.","PV breaker level not clearly  visible, rust stains in the glass tube.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related",12.17,"High","Not Applicable","Not Applicable","PV breaker sight glass dismantled and cleaned.","2021-04-30",null,"Completed","2021-04-21","No",null,null,"Internal"]
[null,null,null,null,null,"103_12/4/2021 3:01:19 PM","2021-04-12","Defect","Ship Staff","Ship Staff Insp.","Port side Fwd Vapour Manifold Valve seat damaged\t","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related",8.17,"Low","Not Applicable","Not Applicable","Spare seat received. Damaged renewed.","2021-05-31",null,"Completed","2021-05-02","No",null,null,"Internal"]
[null,null,null,null,null,"103_12/4/2021 3:07:54 PM","2021-04-12","Defect","Ship Staff","Ship Staff Insp.","Bunker Pipe line near manifold having a soft patch.","Deck - Pipe / Fittings","General Appearance","Equipment Related",6.7,"High","Not Applicable","Not Applicable","Repaired with doubler.","2021-04-30",null,"Completed","2021-04-22","No",null,null,"Internal"]
[null,null,null,null,null,"103_1/5/2021 2:46:05 PM","2021-04-25","Defect","Ship Staff","Ship Staff Insp.","Pin hole leak on boiler feed water line\t","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Leak on the feed line has been rectified.","2021-07-01",null,"Completed","2021-06-04","No",null,null,"Internal"]
[null,null,null,null,null,"103_2/5/2021 8:48:05 PM","2021-05-02","Defect","Ship Staff","Ship Staff Insp.","Both the Anchor chain stoppers are very hard to move.\t","Deck - Mooring Machinery","Mooring","Equipment Related",9.14,"Medium","Not Applicable","Not Applicable","Both the chain stopper freed up.","2021-05-31",null,"Completed","2021-05-22","No",null,null,"Internal"]
[null,null,null,null,null,"103_2/5/2021 8:42:35 PM","2021-05-02","Defect","Ship Staff","Suptd. Insp.","Bridge door having a gap when closed.\t","Accommodation","Safety / LSA / FFA","Equipment Related",5.0999999999999996,"Very High","Not Applicable","Not Applicable","Door packings & locking arrangement  repaired.","2021-05-31",null,"Completed","2021-06-05","No",null,null,"Internal"]

{"sheet":"Calc","index":2,"n_rows":28,"n_cols":12,"rows_kept":28,"cut":false,"hidden":true,"merged":[]}
["Def_type","Def_cause","Equipments","VIQrefno","Observer_code"]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,"Dim itemSele As Long"]
[null,null,null,null,null,null,null,null,null,null,null,"   dim startRow as integer"]
[null,null,null,null,null,null,null,null,null,null,null,"   startRow=1"]
[null,null,null,null,null,null,null,null,null,null,null,"        For itemSele = 0 To ListBox1.ListCount - 1"]
[null,null,null,null,null,null,null,null,null,null,null,"        If ListBox1.Selected(itemSele) = True Then"]
[null,null,null,null,null,null,null,null,null,null,null,"        Worksheets(\"WorksheetName\").Range(\"A\" & startRow).Value = ListBox1.List(itemSele)"]
[null,null,null,null,null,null,null,null,null,null,null,"        startRow = startRow + 1"]
[null,null,null,null,null,null,null,null,null,null,null,"        End If"]
[null,null,null,null,null,null,null,null,null,null,null,"        Next"]
[null,null,null,null,null,null,null,null,null,null,null,"Dim LastRowA As String"]
[null,null,null,null,null,null,null,null,null,null,null,"        Dim itemSele As Long"]
[null,null,null,null,null,null,null,null,null,null,null,"       Dim startRow as integer"]
[null,null,null,null,null,null,null,null,null,null,null,"        LastRowA = ActiveSheet.Cells(Rows.count, \"A\").End(xlUp).row"]
[null,null,null,null,null,null,null,null,null,null,null,"        startQue = 0"]
[null,null,null,null,null,null,null,null,null,null,null,"        For itemSele = 0 To ListBox1.ListCount - 1"]
[null,null,null,null,null,null,null,null,null,null,null,"        For startRow = 1 To LastRowA"]
[null,null,null,null,null,null,null,null,null,null,null,"        If Worksheets(\"WorksheetName\").Range(\"A\" & startRow).Value = ListBox1.List(itemSele) Then"]
[null,null,null,null,null,null,null,null,null,null,null,"        ListBox1.Selected(itemSele) = True"]
[null,null,null,null,null,null,null,null,null,null,null,"        Exit For"]
[null,null,null,null,null,null,null,null,null,null,null,"        End If"]
[null,null,null,null,null,null,null,null,null,null,null,"        Next j"]
[null,null,null,null,null,null,null,null,null,null,null,"        Next"]
[null,null,null,null,null,null,null,null,null,null,null,"        End If"]

{"sheet":"Areaofobs","index":3,"n_rows":17,"n_cols":2,"rows_kept":17,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Cargo / Ballast Systems",11]
["Cert. & Docu.",2]
["Communication",6]
["Crew Management",3]
["Emgcy. Systems",13]
["Eng. / Strg. Comp.",14]
["General Appearance",15]
["Ice Opns.",17]
["ISM Related",7]
["ISPS Related",10]
["MARPOL Related",9]
["MLC Related",4]
["Mooring",12]
["Navigation",5]
["Safety / LSA / FFA",8]
["Structural Condn. / WT integrity ",16]

{"sheet":"Vessel_type","index":4,"n_rows":1,"n_cols":2,"rows_kept":1,"cut":false,"hidden":true,"merged":[]}
["Vessel_type","ID"]

{"sheet":"Deficiency_type","index":5,"n_rows":8,"n_cols":3,"rows_kept":8,"cut":false,"hidden":true,"merged":[]}
["TITLE","Type of deficiency_description","ID"]
["Breakdown",null,6]
["Critical Equipment",null,4]
["Defect",null,1]
["Guarantee Claim",null,8]
["Non Conformity",null,2]
["Observation",null,3]
["Other",null,7]

{"sheet":"VIQrefno","index":6,"n_rows":427,"n_cols":3,"rows_kept":427,"cut":false,"hidden":true,"merged":[]}
["VIQ_ref_no","Risk Value of observation","ID"]
["1.1","Low",8243]
["1.10","Low",8252]
["1.11","Low",8253]
["1.12","Low",8254]
["1.13","Low",8255]
["1.14","Low",8256]
["1.15","Low",8257]
["1.16","Low",8259]
["1.17","Low",8260]
["1.18","Low",8261]
["1.19","Low",8262]
["1.2","Low",8244]
["1.20","Low",8263]
["1.21","Low",8265]
["1.22","Low",8266]
["1.23","Low",8267]
["1.24","Low",8268]
["1.25","Low",8269]
["1.26","Low",8270]
["1.3","Low",8245]
["1.4","Low",8246]
["1.5","Low",8247]
["1.6","Low",8248]
["1.7","Low",8249]
["1.8","Low",8250]
["1.9","Low",8251]
["1.99","High",11258]
["10.1","Medium",8461]
["10.10","High",8470]
["10.11","Medium",8471]
["10.12","Very High",8472]
["10.13","Very High",8473]
["10.14","Medium",8474]
["10.15","Low",8475]
["10.16","Very High",8476]
["10.17","Very High",8477]
["10.18","High",8478]
["10.19","Very High",8479]
["10.2","Low",8462]
["10.20","High",8480]
["10.21","Medium",8481]
["10.22","Low",8482]
["10.23","Medium",8483]
["10.24","Low",8484]
["10.25","Very High",8485]
["10.26","High",8486]
["10.27","Medium",8487]
["10.28","Low",8488]
["10.29","Medium",8489]
["10.3","Medium",8463]
["10.30","High",8490]
["10.31","Very High",8491]
["10.32","Very High",8492]
["10.33","High",8493]
["10.34","High",8494]
["10.35","Very High",8495]
["10.36","Very High",8496]
["10.37","Medium",8497]
["10.38","Medium",8498]
["10.39","High",8499]
["10.4","High",8464]
["10.40","Medium",8500]
["10.41","Medium",8501]
["10.42","Medium",8502]
["10.43","Medium",8503]
["10.44","Medium",8504]
["10.45","Very High",8505]
["10.46","High",8506]
["10.47","Medium",8507]
["10.48","High",8508]
["10.49","Medium",8509]
["10.5","Low",8465]
["10.50","High",8510]
["10.51","Low",8511]
["10.52","Medium",8512]
["10.53","Medium",8513]
["10.54","High",8514]
["10.55","Low",8515]
["10.6","Very High",8466]
["10.7","Medium",8467]
["10.8","Medium",8468]
["10.9","Medium",8469]
["10.99","High",8516]
["11.1","High",8420]
["11.10","Medium",8429]
["11.11","Very High",8430]
["11.12","Low",8431]
["11.13","Low",8432]
["11.14","Medium",8433]
["11.15","Low",8434]
["11.16","Low",8435]
["11.17","Low",8436]
["11.2","Medium",8421]
["11.3","Medium",8422]
["11.4","Very High",8423]
["11.5","Medium",8424]
["11.6","Medium",8425]
["11.7","High",8426]
["11.8","Low",8427]
["11.9","Low",8428]
["11.99","High",8437]
["12.1","High",8438]
["12.10","High",8448]
["12.11","High",8449]
["12.12","High",8450]
["12.13","High",8451]
["12.14","High",8452]
["12.15","High",8453]
["12.16","High",8454]
["12.17","High",8455]
["12.18","High",8456]
["12.19","High",8457]
["12.2","High",8439]
["12.20","High",8458]
["12.21","High",8459]
["12.3","High",8441]
["12.4","High",8442]
["12.5","High",8443]
["12.6","High",8444]
["12.7","High",8445]
["12.8","High",8446]
["12.9","High",8447]
["12.99","High",8460]
["2.1","Very High",8296]
["2.1.9","Very High",11259]
["2.10","Medium",8304]
["2.11","Medium",8305]
["2.12","Low",8306]
["2.13","Low",8307]
["2.14","Low",8308]
["2.15","Low",8309]
["2.16","Medium",8310]
["2.2","Medium",8297]
["2.3","High",8295]
["2.4","Medium",8298]
["2.5","Medium",8299]
["2.6","Low",8300]
["2.7","High",8301]
["2.8","High",8302]
["2.9","Medium",8303]
["2.99","High",8311]
["3.1","High",8312]
["3.2","Very High",8313]
["3.3","High",8314]
["3.4","Low",8294]
["3.5","Medium",8315]
["3.6","High",8316]
["3.7","Very High",8317]
["3.8","Very High",8318]
["3.99","High",8319]
["4.1","High",8320]
["4.10","High",8329]
["4.11","Medium",8330]
["4.12","Very High",8331]
["4.13","Very High",8332]
["4.14","Very High",8333]
["4.15","Very High",8334]
["4.16","Very High",8335]
["4.17","Very High",8336]
["4.18","Very High",8337]
["4.19","Low",8338]
["4.2","Medium",8321]
["4.20","Very High",8339]
["4.21","High",8340]
["4.22","Low",8341]
["4.23","High",8342]
["4.24","High",8343]
["4.25","Low",8344]
["4.26","Low",8345]
["4.27","High",8346]
["4.3","Medium",8322]
["4.4","High",8323]
["4.5","Very High",8324]
["4.6","Medium",8325]
["4.7","High",8326]
["4.8","Medium",8327]
["4.9","Medium",8328]
["4.99","High",8347]
["5.1","Very High",8517]
["5.10","High",8526]
["5.11","Low",8527]
["5.12","Medium",8528]
["5.13","High",8529]
["5.14","Very High",8530]
["5.15","Medium",8531]
["5.16","Very High",8532]
["5.17","Very High",8533]
["5.18","High",8534]
["5.19","Medium",8535]
["5.2","Very High",8518]
["5.20","Medium",8536]
["5.21","Medium",8537]
["5.22","High",8539]
["5.23","Very High",8540]
["5.24","Very High",8541]
["5.25","Medium",8542]
["5.26","Medium",8543]
["5.27","Medium",8544]
["5.28","Very High",8545]
["5.29","High",8546]
["5.3","Low",8519]
["5.30","High",8547]
["5.31","High",8548]
["5.32","High",8549]
["5.33","High",8550]
["5.34","Low",8551]
["5.35","Medium",8552]
["5.36","Low",8553]
["5.37","Low",8554]
["5.38","High",8555]
["5.39","Very High",8556]
["5.4","High",8520]
["5.40","Very High",8557]
["5.41","Very High",8558]
["5.42","Medium",8559]
["5.43","High",8560]
["5.44","High",8561]
["5.45","Medium",8564]
["5.46","Medium",8565]
["5.47","Medium",8566]
["5.48","Medium",8567]
["5.5","Low",8521]
["5.6","Low",8522]
["5.7","Medium",8523]
["5.8","Medium",8524]
["5.9","Very High",8525]
["5.99","High",8568]
["6.1","Medium",8348]
["6.10","Low",8357]
["6.11","High",8358]
["6.12","Medium",8359]
["6.13","Low",8360]
["6.14","High",8361]
["6.15","High",8362]
["6.16","Very High",8363]
["6.17","Very High",8364]
["6.18","Medium",8365]
["6.19","Low",8366]
["6.2","High",8349]
["6.20","Medium",8367]
["6.21","High",8368]
["6.22","Medium",8369]
["6.3","Low",8350]
["6.4","High",8351]
["6.5","Medium",8352]
["6.6","Medium",8353]
["6.7","High",8354]
["6.8","High",8355]
["6.9","Low",8356]
["6.99","High",8370]
["7.1","High",8371]
["7.10","High",8380]
["7.11","High",8381]
["7.12","High",8382]
["7.13","Medium",8383]
["7.14","Medium",8384]
["7.15","High",8385]
["7.16","High",8386]
["7.17","High",8387]
["7.2","High",8372]
["7.3","Low",8373]
["7.4","Low",8374]
["7.5","Low",8375]
["7.6","Medium",8376]
["7.7","Low",8377]
["7.8","High",8378]
["7.9","High",8379]
["7.99","High",8388]
["8.1","Very High",8569]
["8.10","Very High",8578]
["8.100","Low",11227]
["8.101","Medium",11228]
["8.102","Low",11229]
["8.103","Low",11230]
["8.104","Low",11231]
["8.105","Medium",11232]
["8.106","Medium",11233]
["8.107","Low",11234]
["8.108","High",11235]
["8.109","Very High",11236]
["8.11","Medium",8579]
["8.110","High",11237]
["8.111","Medium",11238]
["8.112","High",11239]
["8.113","Medium",11240]
["8.114","Low",11241]
["8.115","High",11242]
["8.116","Medium",11243]
["8.117","Medium",11244]
["8.118","Medium",11245]
["8.119","High",11246]
["8.12","Medium",8580]
["8.120","High",11247]
["8.121","Medium",11248]
["8.122","High",11249]
["8.123","High",11250]
["8.124","Low",11251]
["8.125","High",11252]
["8.126","Medium",11253]
["8.127","Medium",11254]
["8.13","Medium",8581]
["8.14","Very High",8582]
["8.15","High",8583]
["8.16","Very High",8584]
["8.17","Low",8585]
["8.18","High",8586]
["8.19","High",8587]
["8.199","High",11255]
["8.2","Medium",8570]
["8.20","Medium",8588]
["8.21","High",8589]
["8.22","Very High",8590]
["8.23","Medium",8591]
["8.24","Medium",8592]
["8.25","Very High",8593]
["8.26","High",8594]
["8.27","Medium",8595]
["8.28","Medium",8596]
["8.29","High",8598]
["8.3","Very High",8571]
["8.30","High",8599]
["8.31","High",8600]
["8.32","Low",8601]
["8.33","Medium",8602]
["8.34","High",8603]
["8.35","Medium",8604]
["8.36","Medium",8605]
["8.37","High",8607]
["8.38","Medium",8608]
["8.39","Medium",8609]
["8.4","Medium",8572]
["8.40","High",8610]
["8.41","Medium",8611]
["8.42","Medium",8612]
["8.43","Very High",8613]
["8.44","High",8615]
["8.45","High",8616]
["8.46","Very High",8617]
["8.47","Very High",8618]
["8.48","Medium",8619]
["8.49","High",8620]
["8.5","Very High",8573]
["8.50","Medium",8621]
["8.51","Low",8622]
["8.52","Low",8623]
["8.53","Low",8624]
["8.54","High",8625]
["8.55","Low",11182]
["8.56","Medium",11183]
["8.57","Medium",11184]
["8.58","High",11185]
["8.59","High",11186]
["8.6","Medium",8574]
["8.60","High",11187]
["8.61","Medium",11188]
["8.62","Very High",11189]
["8.63","High",11190]
["8.64","Medium",11191]
["8.65","Low",11192]
["8.66","High",11193]
["8.67","High",11194]
["8.68","High",11195]
["8.69","Medium",11196]
["8.7","High",8575]
["8.70","Medium",11197]
["8.71","Very High",11198]
["8.72","Medium",11199]
["8.73","Medium",11200]
["8.74","High",11201]
["8.75","Medium",11202]
["8.76","Medium",11203]
["8.77","Medium",11204]
["8.78","Medium",11205]
["8.79","Medium",11206]
["8.8","Medium",8576]
["8.80","Medium",11207]
["8.81","Low",11208]
["8.82","Medium",11209]
["8.83","Low",11210]
["8.84","Low",11211]
["8.85","Medium",11212]
["8.86","Medium",11213]
["8.87","Medium",11214]
["8.88","Low",11215]
["8.89","High",11216]
["8.9","High",8577]
["8.90","High",11217]
["8.91","High",11218]
["8.92","Medium",11219]
["8.93","Low",11220]
["8.94","Low",11221]
["8.95","Medium",11222]
["8.96","Medium",11223]
["8.97","Low",11224]
["8.98","High",11225]
["8.99","Medium",11226]
["9.1","Low",8390]
["9.10","Medium",8399]
["9.11","Medium",8400]
["9.12","Medium",8401]
["9.13","Low",8402]
["9.14","Medium",8403]
["9.15","Medium",8404]
["9.16","High",8405]
["9.17","High",8406]
["9.18","Low",8407]
["9.19","Low",8408]
["9.2","Very High",8391]
["9.20","Medium",8409]
["9.21","Medium",8410]
["9.22","Low",8411]
["9.23","Low",8412]
["9.24","Medium",8413]
["9.25","Low",8414]
["9.26","Low",8415]
["9.27","Low",8416]
["9.28","Medium",8417]
["9.29","Low",8418]
["9.3","Very High",8392]
["9.4","High",8393]
["9.5","High",8394]
["9.6","Low",8395]
["9.7","Medium",8396]
["9.8","Medium",8397]
["9.9","Medium",8398]
["9.99","High",8419]

{"sheet":"Equipment_list","index":7,"n_rows":28,"n_cols":3,"rows_kept":28,"cut":false,"hidden":true,"merged":[]}
["TITLE","Equipment_list_description","ID"]
["Accommodation",null,12]
["Cargo Mach.",null,13]
["Critical Equip.",null,16]
["Deck - Machinery",null,18]
["Deck - Mooring Machinery",null,15]
["Deck - Pipe / Fittings",null,20]
["Documentation",null,21]
["E/R - Air Comp.",null,8]
["E/R - Aux. Engine",null,4]
["E/R - Aux. Mach.",null,7]
["E/R - Boiler",null,5]
["E/R - Main Engine",null,3]
["E/R - Pipes/ valves & fittings",null,9]
["E/R - Pumps",null,32]
["E/R - Purifier",null,6]
["Elect. Mach. & Equip.",null,10]
["Hull & Tanks",null,19]
["Inert Gas",null,14]
["LSA / FFA",null,17]
["Miscellaneous",null,22]
["Navigation - DGPS / EPFS / AIS",null,28]
["Navigation - ECDIS",null,25]
["Navigation - Echo Sounder / Speed Log",null,26]
["Navigation - GMDSS & Communication",null,23]
["Navigation - Others",null,11]
["Navigation - RADAR",null,24]
["Navigation - VDR / BNWAS",null,30]

{"sheet":"PSC_MOU","index":8,"n_rows":11,"n_cols":3,"rows_kept":11,"cut":false,"hidden":true,"merged":[]}
["TITLE","PSC_MOU_description","ID"]
["Asia and the Pacific",null,2]
["Caribbean",null,4]
["Europe and the North Atlantic",null,1]
["Latin America",null,3]
["The Black Sea region",null,6]
["The Indian Ocean",null,8]
["The Mediterranean",null,7]
["The Riyadh MoU",null,9]
["USCG",null,10]
["West and Central Africa",null,5]

{"sheet":"Inspection_type","index":9,"n_rows":13,"n_cols":2,"rows_kept":13,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Bunkering Audit",14]
["Cargo Audit",17]
["Engineering Audit",16]
["ISM Audit",2]
["ISPS Audit",3]
["IT Audit",10]
["MLC Audit",1]
["Mooring Audit",9]
["Nav Audit / Verification",8]
["Onboard Training",18]
["Ship Staff Insp.",15]
["Suptd. Insp.",13]

{"sheet":"Deficiency_Cause","index":10,"n_rows":8,"n_cols":3,"rows_kept":8,"cut":false,"hidden":true,"merged":[]}
["TITLE","Deficiency_Cause_description","ID"]
["Behaviour Based",null,1]
["Equipment Related",null,4]
["External Factors",null,5]
["Human Error",null,7]
["Inappropriate Procedure",null,8]
["Industry Issue",null,6]
["Knowledge Based",null,3]

{"sheet":"Observer_code","index":11,"n_rows":3,"n_cols":3,"rows_kept":3,"cut":false,"hidden":true,"merged":[]}
["TITLE","Observer_code_description","ID"]
["Owner / Marine / Tech. Suptd.",null,3]
["Ship Staff",null,2]

{"sheet":"Status_code","index":12,"n_rows":6,"n_cols":3,"rows_kept":6,"cut":false,"hidden":true,"merged":[]}
["TITLE","Status_code_description","ID"]
["Completed",null,6]
["Deferred to D D",null,5]
["In progress",null,3]
["Not Started",null,2]
["Waiting spare",null,4]

{"sheet":"PSC_ref_no","index":13,"n_rows":19,"n_cols":2,"rows_kept":19,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Alarms",9]
["Cargo operations including equipment",7]
["Certificates & Documentation",2]
["Dangerous Goods",13]
["Emergency Systems",5]
["Fire safety",8]
["ISM",16]
["ISPS",17]
["Life saving appliances",12]
["MLC, 2006",18]
["Other",19]
["Pollution Prevention",15]
["Propulsion and auxiliary machinery",14]
["Radio communication",6]
["Safety of Navigation",11]
["Structural condition",3]
["Water/Weathertight condition",4]
["Working and Living Conditions",10]

{"sheet":"Risk_value_of_obs","index":14,"n_rows":1,"n_cols":2,"rows_kept":1,"cut":false,"hidden":true,"merged":[]}
["Risk Value of observation","ID"]

{"sheet":"Year","index":15,"n_rows":18,"n_cols":1,"rows_kept":18,"cut":false,"hidden":true,"merged":[]}
["Year"]
[2014]
[2015]
[2016]
[2017]
[2018]
[2019]
[2020]
[2021]
[2022]
[2023]
[2024]
[2025]
[2026]
[2027]
[2028]
[2029]
[2030]

{"sheet":"Month","index":16,"n_rows":13,"n_cols":1,"rows_kept":13,"cut":false,"hidden":true,"merged":[]}
["Month"]
["Jan"]
["Feb"]
["Mar"]
["Apr"]
["May"]
["Jun"]
["Jul"]
["Aug"]
["Sep"]
["Oct"]
["Nov"]
["Dec"]

{"sheet":"Date_","index":17,"n_rows":32,"n_cols":1,"rows_kept":32,"cut":false,"hidden":true,"merged":[]}
["Date"]
["01"]
["02"]
["03"]
["04"]
["05"]
["06"]
["07"]
["08"]
["09"]
[10]
[11]
[12]
[13]
[14]
[15]
[16]
[17]
[18]
[19]
[20]
[21]
[22]
[23]
[24]
[25]
[26]
[27]
[28]
[29]
[30]
[31]

{"sheet":"Sheet1","index":18,"n_rows":24,"n_cols":6,"rows_kept":24,"cut":false,"hidden":true,"merged":[]}
[]
[null,"ID","E",null,"Date Recorded",1]
[null,"UNIQUE ID","F",null,"Type of Deficiency",2]
[1,"Date Recorded","G",null,"Observer code",3]
["ignore","Vessel Type","H",null,"Type of Inspection",4]
[null,"Internal / External","I",null,"Description of Deficiency",5]
[null,"Drydock","J",null,"Equipment Categories",6]
[null,"Information Sharing","K",null,"Area of Observation",7]
[null,"Critical_item","L",null,"Deficiency Cause",8]
[null,"Deficiency Type","M",null,"VIQ Ref Number",9]
[null,"Deficiency Cause","N",null,"Risk Value of Obs",10]
[null,"Inspection Type","O",null,"PSC Ref Number",11]
[null,"Equipments","P",null,"PSC MOU ID",12]
[null,"VIQ Reference Number","Q",null,"Action Taken or Required",13]
[null,"Risk Value of the observation","R",null,"Target Date",14]
[null,"PSC Reference Number","S",null,"PO Ref No.",15]
[null,"PSC MOU","T",null,"Status Code",16]
[null,"Observer Code","U",null,"Date Completed",17]
[null,"Target Date","V",null,"Drydock",18]
[null,"Status Code","W",null,"Info Sharing",19]
[null,"Description of Deficiency","X",null,"Critical Item Flag",20]
[null,"Action taken / required","Y",null,"Audit Type",21]
[null,"PO ref no","Z"]
[null,"Date completed","AA"]

{"sheet":"Ship_information","index":19,"n_rows":2,"n_cols":3,"rows_kept":2,"cut":false,"hidden":true,"merged":[]}
["Ship_ID","Ship_Name","FILE_NAME"]
["103","GILOS (16-03-2021)","103_1615890932465.xlsm"]

{"sheet":"External_Deficiency_type","index":20,"n_rows":5,"n_cols":3,"rows_kept":5,"cut":false,"hidden":true,"merged":[]}
["TITLE","Type of deficiency_description","ID"]
["Condn of Class / Memo",null,5]
["Defect",null,1]
["Non Conformity",null,2]
["Observation",null,3]

{"sheet":"External_Inspection_type","index":21,"n_rows":11,"n_cols":2,"rows_kept":11,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Cargo Audit",17]
["Flag State Insp.",5]
["ISM Audit",2]
["ISPS Audit",3]
["MLC Audit",1]
["Nav Audit / Verification",8]
["OM Insp. (Eg. SIRE / CDI etc.)",6]
["Others (Eg. Insurance etc.)",12]
["PSC Inspection",4]
["Terminal Insp.",11]

{"sheet":"External_Observer_code","index":22,"n_rows":7,"n_cols":3,"rows_kept":7,"cut":false,"hidden":true,"merged":[]}
["TITLE","Observer_code_description","ID"]
["Class Surveyor",null,4]
["FSC Inspector",null,5]
["Others (Eg. Insurance etc.)",null,9]
["PSC Insp.",null,6]
["SIRE / CDI Insp.",null,8]
["Terminal Insp.",null,7]

{"sheet":"Sheet Version","index":23,"n_rows":2,"n_cols":2,"rows_kept":2,"cut":false,"hidden":true,"merged":[]}
["Version","Title"]
["2.0","Version 2.0"]