{"text_format":"1","workbook":"xlsx","n_sheets":24,"sheets":["Mainsheet","Completed","Calc","Areaofobs","Vessel_type","Deficiency_type","VIQrefno","Equipment_list","PSC_MOU","Inspection_type","Deficiency_Cause","Observer_code","Status_code","PSC_ref_no","Risk_value_of_obs","Year","Month","Date_","Sheet1","Ship_information","External_Deficiency_type","External_Inspection_type","External_Observer_code","Sheet Version"],"not_rendered":{"charts":0,"images":5,"macros":1,"external_links":0,"defined_names":12,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Mainsheet","index":0,"n_rows":45,"n_cols":28,"rows_kept":45,"cut":false,"hidden":false,"merged":[[10,8,10,9],[10,12,10,13],[12,6,12,27],[8,6,8,27]]}
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,"Defect - Damage Monitoring Sheet"]
[]
[null,null,null,null,null,null,null,"Date of Report","06-Aug-2021",null,null,"Ship Name","DHT FALCON (06-08-2021)"]
[]
[null,null,null,null,null,null,"VERSION : 2.0"]
[]
[]
[]
[null,null,null,null,"ID","UNIQUE ID","Date Recorded","Type of Deficiency","Observer code","Type of Inspection","Description of Deficiency","Equipment Categories","Area of Observation","Deficiency Cause","VIQ Ref Number","Risk Value of Obs","PSC Ref Number","PSC MOU ID","Action Taken or Required","Target Date","PO Ref No.","Status Code","Date Completed","Drydock","Info Sharing","Critical Item","Audit Type","Superintendent Remarks"]
[null,null,null,null,17788,"22_09/02/2021 1:31:21 PM","2021-03-02","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Several minor steel works on deck to be numbered and included in the docking repairs.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related",11.4,"Very High","Not Applicable","Not Applicable","Pipe to be renewed during dry docking. SEVERAL STELL RENEWAL JOB RAISED IN REFMAN.","2021-09-30",null,"Deferred to D D",null,"Yes","No","No","Internal","DD job / to be planned for the 3rd special mid 2021 - refman job to be created\nvessel to revert after marking, numbering and physical details for the refman data."]
[null,null,null,null,13953,"22_16/09/2020 12:47:44 PM","2021-02-22","Observation","Ship Staff","Ship Staff Insp.","Low insulation fault from scrubber booster pump VFD panel.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.38","Medium","","","Noted one time insulation fault occured from the VFD","2021-08-31","","In progress",null,"No","No","No","Internal","leave it open for warrenty issues. No issues at present\nwarrenty closed in Jan 2021"]
[null,null,null,null,17789,"22_09/02/2021 1:32:59 PM","2021-03-02","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Self-closing Springs on the ballast water tank sounding pipes, few of them in poor condition","Hull & Tanks","Cargo / Ballast Systems","Equipment Related","10.26","High","","","Defectibe self closing spring to be renewed. CHIPPING / PAINTING JOB DONE SOME OF THE SOUNDING PIPES, SELF CLOSING HANDLE MADE FREE, DURING CHIPPING SOME OF THE SOUNDING PIPE HOLED, NEED TO CARRY OUT FABRICATION JOB DURING DD, RO FOR SPRINGS TO BE RAISED IN DUE COURSE.","2021-10-31","VESSEL RECEIVED DFAL210193 : SPRING FOR CARGO/BALLAST SAMPLING PIPE CLOSING ARRANGEMENT. VESSEL WILL","Deferred to D D",null,"No","No","No","Internal","easy job; to be closed on priority.\nraise RO for springs"]
[null,null,null,null,18222,"22_09/03/2021 5:51:43 PM","2021-03-05","Defect","Ship Staff","Ship Staff Insp.","ATMOSPHERIC CONDENSER PERFORMANCE IS VERY POOR.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","NEW CONDESNER RECEIVED. JOB DEFERRED TO DD","2021-10-10","","Deferred to D D",null,"Yes","No","No","Internal","spare reconditioned condenser connected onboard - replace it if suitable anchorage before loading."]
[null,null,null,null,18224,"22_09/03/2021 5:49:13 PM","2021-03-09","Observation","Ship Staff","Ship Staff Insp.","FRESH WATER GENERATOR CONDENSER 4 NOS OF TUBES WERE FOUND LEAKING.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","LEAKING TUBES PLUGGED. TOTAL 7 NOS OF TUBES WERE PLUGGED SO FAR. PLUGGED TUBES TO BE RENEWED.","2021-10-10","","Deferred to D D",null,"Yes","No","No","Internal","Please include the job under DDRL for condenser retubing at the forth coming docking. raise Ro for the tubes."]
[null,null,null,null,18401,"22_26/03/2021 3:26:00 PM","2021-03-22","Defect,Observation","Ship Staff","Ship Staff Insp.","AUX ENGINE NO 3 COOLING WATER LINE VALVE IS WRONG. IT IS FITTED WITH NORMAL VALVE INSTEAD OF NON RETURN VALVE. THIS CAUSES WATER TO BE RECIRCULATED IN THE GENERATOR AND AFFECTING THE PERFORMANCE OF OTHER GENERATORS","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","VALVE TO BE REPLACED WITH NRV. SPARE TO BE ORDERED. THIS JOB CAN BE DONE ONLY DURING BALCKOUT AS COOLING SYSTEM OF ALL AE ARE IN A LOOP","2021-10-10","","Deferred to D D",null,"No","No","No","Internal","id the spare correct type valve available for change. then complete the job as planned.\notherwise raise RO for Singapore. vessel may have waiting time in China. seek office approval once ready for job with correct RA."]
[null,null,null,null,18403,"22_31/03/2021 10:40:27 AM","2021-03-28","Defect","Ship Staff","Ship Staff Insp.","MAIN SEA WATER PUMP PRIMING PUMP IS DEEFCTIVE. PRIMING PUMP TO BE OVERHAULED. SUCTION VALVE OF THE PUMP IS NOT HOLDING.BLACK OUT JOB","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","MAIN SEA WATER PUMP PRIMING PUMP IS DEEFCTIVE. PRIMING PUMP TO BE OVERHAULED. SUCTION VALVE OF THE PUMP IS NOT HOLDING.BLACK OUT JOB","2021-10-10","","Deferred to D D",null,"Yes","No","No","Internal","Kindly plan the job in ballast leg at suitable anchorage.\nOr include in the forthcoming docking in Mid 2021.\nforward the refman export"]
[null,null,null,null,18225,"22_10/03/2021 11:25:07 AM","2021-03-31","Observation","Ship Staff","Ship Staff Insp.","No Spare o rings available onboard for FO and LO pump strainers.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related",10.19,"Very High","Not Applicable","Not Applicable","RO raised. O-Rings to be renewed once spares received.","2021-09-10","DFAL 210081","Waiting spare",null,"No","No","No","Internal","spares to be arranged as per the request."]
[null,null,null,null,18994,"22_3/4/2021 15:18:00","2021-04-01","Defect","Ship Staff","Ship Staff Insp.","Mushroom vent top for Galley Exh on B Deck Stbd is separated. ","Deck - Machinery","Structural Condn. / WT integrity ","External Factors","11.7","High","","","Repair/replacement involving fabrication of securing arragement","2021-08-30","","Deferred to D D",null,"No","No","No","Internal"]
[null,null,null,null,18996,"22_05/04/2021 7:13:09 PM","2021-04-05","Defect","Ship Staff","Suptd. Insp.","BOTH BOILERS REFRACTORY DAMAGE NOTED AT SWIRLER AREA","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","TEMPORARY REPAIR CARRIED OUT. PERMANANT REPAIR TO BE DONE AT DRYDOCK","2021-09-11","","Deferred to D D",null,"Yes","No","No","Internal","refractory around furnace tube walls to be checked and repaired after every cargo operations.  anchor points to be renewed during docking"]
[null,null,null,null,18997,"22_23/04/2021 9:31:10 AM","2021-04-16","Defect","Ship Staff","Ship Staff Insp.","AUX ENGINE FO STEAM TRACING LINE LEAKING. PIPE HAS NO FLANGES NEARBY AND SLEEVE JOINED. HENCE DIFFICULT TO REMOVE THE PIPE WHEN BOILERS OR EGB IN OPERATION","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","LEAKING SECTION OF THE PIPE TO BE RENEWED.","2021-09-11","","Deferred to D D",null,"No","No","No","Internal","carry out temp repairs for now and plan renewal during the upcoming docking"]
[null,null,null,null,18999,"22_30/04/2021 9:26:01 AM","2021-04-22","Defect","Ship Staff","Ship Staff Insp.","ENGINE ROOM ENTRANCE DOOR FROM UPPER DECK TO BE REPAIRED","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.32","High","","","DOOR HINGES TIGHTENED, NEED TO REPLACE DOOR AND ADJUST FRAME.","2021-09-11","","In progress",null,"No","No","No","Internal","complete as planned and close out"]
[null,null,null,null,19001,"22_30/04/2021 9:30:45 AM","2021-04-25","Defect","Ship Staff","Ship Staff Insp.","TOILET FLUSH OF FEW CABIN ARE DEFECTIVE","Miscellaneous","MLC Related","Equipment Related","8.55","Low","","","FLUSH SYSTEM TO BE RENEWED. NEED TO ORDER SPARES. WILL RAISE RO SHORTLY.","2021-08-31","","Not Started",null,"No","No","No","Internal","is there any RO, \nmention the RO number in DDRL and follow up"]
[null,null,null,null,19453,"22_14/05/2021 9:27:44 AM","2021-05-07","Defect","Ship Staff","Ship Staff Insp.","CORROSION AND MATERIAL WASTAGE NOTED AT CASCADE TANK TOP AREA","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","CORRODED PLATED TO BE RENEWED DURING DD","2021-09-07","","Deferred to D D",null,"Yes","No","No","Internal","job in DD specs for completion while docking in Aug21"]
[null,null,null,null,19455,"22_14/05/2021 9:44:49 AM","2021-05-10","Defect","Ship Staff","Ship Staff Insp.","TANK CLEANING PUMP REMOTE TRIP AND OTHER TRIPS SOLENOID IS DEFECTIVE","Cargo Mach.","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","NEW SOLENOID RECEIVED AT SINGAPORE ON 11/07/21. PLANNING TO CARRY OUT THE JOB IN LOADED PASSAGE BEFORE CARGO LINE PRESSURE TEST.","2021-08-25","DFAL 210146","In progress",null,"No","No","No","Internal","spares confirmed with shinko, awaiting supply. follow up with procure"]
[null,null,null,null,18223,"22_09/03/2021 5:47:17 PM","2021-05-13","Defect","Ship Staff","Ship Staff Insp.","IGS EXCESS DUMP VALVE E/P CONVERTOR DEFECTIVE","Cargo Mach.","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","AS PER CONVERTOR SUPPLIER TECHNICIAN WILL ATTEND THE JOB IN DRY DOCK","2021-09-20",null,"Deferred to D D",null,"Yes","No","No","Internal","spares confirmed with Kuidatech for spares/ please confirm if the issue resolved after remote troubleshooting. follow up please"]
[null,null,null,null,19727,"22_6/15/2021 4:06:39 AM","2021-06-06","Defect","Ship Staff","Ship Staff Insp.","Inert Gas regulating valve not operating in auto mode to maintain set pressure in cargo tanks during cargo discharging/COW operation.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related",8.2200000000000006,"Very High","Not Applicable","Not Applicable","ALREADY WORKED ON AND ADJUSTED , WILL TRY OUT DURING PRESSURE TESTING OF CARGO LINE BEFORE DISCHARGING.","2021-08-25",null,"In progress",null,"No","No","No","Internal","awaiting details. \nServ also included under docking automation service.\nrevert with the RO for the sensing unit on priority"]
[null,null,null,null,19728,"22_6/15/2021 6:12:52 AM","2021-06-06","Defect","Ship Staff","Ship Staff Insp.","FPK ballast tank sounding gauge in CCR not operatioanal.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.12","Medium","","","Vessel staff renewed purge unit of FPK ballast tank sounding gauge, still no reading was shown in CCR. Pipe line from CCR to tank to be thorughly checked and leak to be rectified. ","2021-09-30","","In progress",null,"No","No","No","Internal","include in additional docking jobs ; use the ref no and forward to office"]
[null,null,null,null,19729,"22_6/17/2021 1:03:09 AM","2021-06-06","Breakdown","Ship Staff","Ship Staff Insp.","Vessel is equipped with 2 hydroblasters for deck maintenance. Both hydroblaster are presently inoperational. One hydroblaster nozzle damaged, awaiting spare. Other hydroblaster tripping due to overload and slight water leakage from hose connection.","Deck - Machinery","General Appearance","Equipment Related","","","","","Vessel awaiting spare for one hydroblaster RO DFAL210157. For 2nd hydroblaster, issue pending investigation.","2021-09-30"," RO DFAL210157","Waiting spare",null,"No","No","No","Internal","spares processed; revert with condition of second blaster in mail."]
[null,null,null,null,19730,"22_15/06/2021 6:11:03 PM","2021-06-08","Other","Ship Staff","Ship Staff Insp.","IN/OUT SECTION OF ME & AE COOLER SEA WATER LINES CORRODED AND LEAKING.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","11.4","Very High","","","TEMPORARILY REPAIRED AND ADDED IN DD SPECS.","2021-09-30","","Deferred to D D",null,"Yes","No","No","Internal","forward additional specs for docking.\nplanned renewal during docking"]
[null,null,null,null,19937,"22_7/1/2021 6:52:29 AM","2021-06-29","Other","Ship Staff","Ship Staff Insp.","During cargo stripping operation, it was observed COP and TCP casing drain valves on 50mm pipe line SRV-800, SRV-801 & SRV-803 valve spindles broken, valves spindle keep rotating and no change in valve status (Open/Shut) observed.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.11","Medium","","","Vessel replaced valve SRV 801. Remaining valve will be replaced during next ballast passage or during docking.","2021-09-30","Vessel received valves for replacement DFAL210174.","In progress",null,"No","No","No","Internal","plan renewal and close out.\nif unable to complete then must be done during DD."]
[null,null,null,null,20150,"22_21/07/2021 7:07:15 PM","2021-07-13","Other","Ship Staff","Ship Staff Insp.","VARIOUS STEAM LEAKS IN ENGINE ROOM M/E F.O. HEATER TRACING STEAM LINE LEAKING , HFO BUNKER TANK STEAM RETURN LINE ","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","TO REPAIR PIPELINE BY WELDING / RENEW PIPE SECTION","2021-09-11",null,"Deferred to D D",null,"No","No","No","Internal","complete as planned and close out"]
[null,null,null,null,20329,"22_7/24/2021 8:34:06 AM","2021-07-23","Defect","Ship Staff","Ship Staff Insp.","Cargo stripping pump water leakage from steam chest continuosly, when stripping pump not in use. Cargo stripping pump relief valve, slight oil leakage.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.11","Medium","","","Investigation under progress.","2021-09-30","","In progress",null,"No","No","No","Internal","check auto valve and isolation valves// the drains are also not open. report in separate mail."]
[null,null,null,null,20330,"22_05/08/2021 11:19:56 PM","2021-07-29","Other","Ship Staff","Ship Staff Insp.","LEAK IN STEAM RETURN LINE FROM WASTE OIL SERVICE TANK (INCINERATOR)","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","NEED TO RMOVE THE PIPE SECTION AND RENEW IT. JOB TO BE DONE IN DD","2021-09-11","","Deferred to D D",null,"No","No","No","Internal","include in the additional list with all the material details and pipe section details . forward the updated excel sheet"]
[null,null,null,null,20331,"22_05/08/2021 10:02:11 PM","2021-07-30","Other","Ship Staff","Ship Staff Insp.","Sea water cooling return line for accomodation A/C condensor leaking.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Temporary repairs carried out.Need to stop accomodation A/C and remove the pipe section and repair by welding in workshop.Job planned prior discharging port as expecting ambient temperature to drop and can stop A/C.","2021-08-26",null,"Not Started",null,"No","No","No","Internal","Plan renewal in DD.. include in additional repairs list and forward me the updated list"]
[null,null,null,null,20332,"22_8/3/2021 8:21:41 AM","2021-08-03","Defect","Ship Staff","Ship Staff Insp.","M5 mooring winch aft,  wire in strand found broken near eye and small kink also developed in middle length of wire. Wire has eye onle at ene end and other end is plane. Vessel can not change end to end after 5 years of service. Wire certificate no. 09-s-008567. Length-300Mtr","Deck - Mooring Machinery","Mooring","Equipment Related",9.17,"High","Not Applicable","Not Applicable","Wire has to be offlanded at dock, eye end to be cropped and new eyes with mechanical splice to be fabricated. ","2021-09-30",null,"In progress",null,"No","No","No","External"]
[null,null,null,null,null,"22_8/18/2021 2:38:13 AM","2021-08-08","Defect","Ship Staff","Ship Staff Insp.","Vessel was changing direction of mooring wire end to end for M2-B, observed few wire strands broken (4-5) at end of eye. ","Deck - Mooring Machinery","Mooring","Equipment Related",9.17,"High","Not Applicable","Not Applicable","Damage eye of mooring wire required to be cropped, new eye to be fabricated with mechanical splice.","2021-10-10",null,"In progress",null,"No",null,null,"Internal"]
[null,null,null,null,null,"22_21/08/2021 3:01:41 PM","2021-08-09","Other","Ship Staff","Ship Staff Insp.","LEAK ON S.W. SERVICE PUMP DISCHARGE LINE TO MGPS","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","VALVE NOT HOLDING. TEMPORARY REPAIR CARRIED OUT. WILL CARRY OUT JOB IN DD","2021-09-21",null,"Deferred to D D",null,"Yes",null,null,"Internal"]

{"sheet":"Completed","index":1,"n_rows":409,"n_cols":28,"rows_kept":409,"cut":false,"hidden":false,"merged":[[10,8,10,9],[10,12,10,13],[12,6,12,27],[8,6,8,27]]}
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,"Defect - Damage Monitoring Sheet"]
[]
[null,null,null,null,null,null,null,"Date of Report","06-Aug-2021",null,null,"Ship Name","DHT FALCON (06-08-2021)"]
[]
[null,null,null,null,null,null,"VERSION : 2.0"]
[]
[]
[]
[null,null,null,null,"ID","UNIQUE ID","Date Recorded","Type of Deficiency","Observer code","Type of Inspection","Description of Deficiency","Equipment Categories","Area of Observation","Deficiency Cause","VIQ Ref Number","Risk Value of Obs","PSC Ref Number","PSC MOU ID","Action Taken or Required","Target Date","PO Ref No.","Status Code","Date Completed","Drydock","Info Sharing","Critical Item","Audit Type","Superintendent Remarks"]
[null,null,null,null,2749,"22_19/10/2019 1:40:25 AM","2018-07-07","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ME unit #1 exhaust valve top cover oil leakage from gasket to rectify.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.1","Medium","","","ME unit #1 exhaust valve top cover gasket replaced with new one. No further leaks.","2018-07-31","","Completed","2019-07-12","No","No","No","Internal"]
[null,null,null,null,2748,"22_19/10/2019 1:37:11 AM","2018-11-07","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Broken vent valve on Low sea chest to renew","E/R - Pipes/ valves & fittings","Cargo / Ballast Systems","Equipment Related","8.2","Medium","","","Broken vent valve replaced with new valve.","2019-07-31","","Completed","2019-07-17","No","No","No","Internal"]
[null,null,null,null,2750,"22_19/10/2019 1:42:07 AM","2018-11-07","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ME fuel line high pressure pipes to be protected with Anti splash tape","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.8","Medium","","","Anti splash tape fitted on high pressure pipe connections.","2019-07-31","","Completed","2019-07-30","No","No","No","Internal"]
[null,null,null,null,2751,"22_19/10/2019 1:43:47 AM","2018-11-07","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ME fuel pump shaft bearing and linkage to be greased.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.8","Medium","","","Main engine all unit pump shaft and linkages lubricated. Regular lubrication is being done on weekly basis.","2019-07-31","","Completed","2019-07-30","No","No","No","Internal"]
[null,null,null,null,2752,"22_19/10/2019 1:44:57 AM","2018-11-07","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Control Air Leakage from VIT Actuator Control Unit to be rectified.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.2","Low","","","Lak rectified","2019-08-15","","Completed","2019-07-12","No","No","No","Internal"]
[null,null,null,null,2753,"22_19/10/2019 1:46:29 AM","2018-11-07","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Numerous lights inside Engine casing not working","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.2","Low","","","fused lightings has been replaced with new one.","2019-07-31","","Completed","2019-08-21","No","No","No","Internal"]
[null,null,null,null,2754,"22_19/10/2019 1:47:51 AM","2018-11-07","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","FO Supply Pump No.1 & 2 Suction Pressure Gauge to be renewed.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.8","Medium","","","pressure gauge renewed.","2019-07-31","","Completed","2019-08-02","No","No","No","Internal"]
[null,null,null,null,2755,"22_19/10/2019 1:49:07 AM","2018-11-07","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Steering Gear LO Storage Tank Minimum Level Marking as per SOLAS missing. ","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.2","Low","","","Minimum level has been marked with stencils.","2019-07-15","","Completed","2019-07-12","No","No","No","Internal"]
[null,null,null,null,2756,"22_19/10/2019 1:51:30 AM","2018-11-07","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","A/E Performance report indicates :-\n\nA/E 1 Unit #3 Fuel Injector to overhaul.\n\nA/E 2 Unit #4 Fuel Injector to overhaul. \n\nC/E to take corrective action\n\n","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.2","Low","","","AE #1 unit 3 fuel injector removed and overhauled. AE #2 unit 4 fuel injector removed and overhauled.","2019-08-31","","Completed","2019-08-14","No","No","No","Internal"]
[null,null,null,null,2757,"22_19/10/2019 1:55:45 AM","2018-11-07","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ME performance report indicates power imbalance between unit #3 and #7. C/E to take corrective action.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.2","Low","","","completed. Performance marked.","2019-08-31","","Completed","2019-08-16","No","No","No","Internal"]
[null,null,null,null,2758,"22_19/10/2019 1:57:09 AM","2018-11-07","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","AHU room to be arranged.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.2","Low","","","completed.","2019-07-31","","Completed","2019-07-30","No","No","No","Internal"]
[null,null,null,null,2759,"22_19/10/2019 1:58:39 AM","2018-11-07","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","numerous lagging missing/ damaged in E/R, same to be renewed","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.2","Low","","","damaged lagging has been replaced with new lagging.","2019-08-15","","Completed","2019-08-06","No","No","No","Internal"]
[null,null,null,null,2760,"22_19/10/2019 2:19:42 AM","2018-11-07","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Engine/ electrical spares store room to be arranged","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.2","Low","","","Stores arranged.","2019-08-15","","Completed","2019-07-30","No","No","No","Internal"]
[null,null,null,null,2762,"22_19/10/2019 2:22:37 AM","2018-11-07","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Spares inventory to be updated in PAL","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.2","Low","","","Inventory checked and updated.","2019-07-31","","Completed","2019-08-21","No","No","No","Internal"]
[null,null,null,null,2644,"22_17/10/2019 5:42:47 AM","2019-01-01","Defect","Owner / Marine / Tech. Suptd.","Ship Staff Insp.","Seepage in both lifeboats from remote wire opening","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.27","Medium","","","Silicone has been put in opening to avoid rain water ingress & checked for water integrity","2019-09-03","","Completed","2019-03-10","No","No","No","Internal"]
[null,null,null,null,2646,"22_17/10/2019 5:54:26 AM","2019-01-03","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Hydroblaster to be overhauled on priority and put in use.","Miscellaneous","General Appearance","Equipment Related","11.7","High","","","Rupture disc replaced with the available spares & hydroblaster put in use.","2019-03-15","DFAL190072","Completed","2019-03-11","No","No","No","Internal"]
[null,null,null,null,2667,"22_2019-10-17 07:22:08.000","2019-01-03","Defect","Ship Staff","Ship Staff Insp.","Main engine control air pressure gauge to renew","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.21","Medium","","","The defective pressure gauge renewed","2019-03-31","","Completed","2019-03-09","No","No","No","Internal"]
[null,null,null,null,2692,"22_18/10/2019 2:21:57 AM","2019-01-04","Defect","Ship Staff","Ship Staff Insp.","EGE feed pump No. 2 not developing sufficient pressure.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.2","Low","","","The pump overhauled, all the mouth rings renewed. Now the pump performance is satisfactory.","2019-04-20","","Completed","2019-04-04","No","No","No","Internal"]
[null,null,null,null,2693,"22_18/10/2019 2:23:38 AM","2019-01-04","Defect","Ship Staff","Ship Staff Insp.","Aux boiler No. 2 water outlet valve to circulating pump leaking from gland packing","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.8","Medium","","","The boiler depressurised and gland packing renewed.","2019-04-15","","Completed","2019-04-03","No","No","No","Internal"]
[null,null,null,null,2732,"22_19/10/2019 12:54:45 AM","2019-01-04","Defect","Ship Staff","Ship Staff Insp.","Waste oil incinerator display not clear","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.2","Low","","","New display unit received, same fitted in place. Tried out, working satisfactory.","2019-06-15","","Completed","2019-06-14","No","No","No","Internal"]
[null,null,null,null,8684,"22_Fri Dec 20 2019 23:51:51 GMT+0000 (Coordinated Universal Time)","2019-01-08","Defect","Ship Staff","Ship Staff Insp.","Accommodation block underside of bridge wings to be derusted and painted","Accommodation","General Appearance","Equipment Related","11.7","High","","","Vessel completed both side underside bridge wings","2019-10-15","","Completed","2019-11-15","No","No","No","Internal"]
[null,null,null,null,9963,"22_1/20/2020 2:14:05 PM","2019-01-21","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Some of the entries of Echo Sounder running scale were missing in Deck Log Book. ","Navigation - Others","Navigation","Inappropriate Procedure","4.7","High","","","Discussed with all navigating officer’s & emphasized on to follow the company’s procedure’s correctly at all times.","2019-01-23","","Completed","2019-01-22","No","No","No","Internal"]
[null,null,null,null,9964,"22_1/20/2020 2:16:05 PM","2019-01-21","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Few compass error missing, after wide alteration of course by more than 20 Degrees, Compass error was not calculated and recorded in Deck Log Book.","Navigation - Others","Navigation","Human Error","4.9","Medium","","","Discussed with all navigating officer’s & emphasized on to follow the company’s procedure’s correctly at all times.","2019-01-30","","Completed","2019-01-29","No","No","No","Internal"]
[null,null,null,null,9971,"22_1/20/2020 2:12:12 PM","2019-01-21","Observation","Owner / Marine / Tech. Suptd.","Ship Staff Insp.","DURING ANCHORAGE NEAREST LANDMARK (NAME AND RANGE,BEARING) WAS MISSING IN DECK LOG BOOK.","Navigation - Others","Crew Management","Inappropriate Procedure","4.2","Medium","","","Discussed with all navigating officer’s & emphasized on to follow the company’s procedure’s correctly at all times.","2019-01-23","","Completed","2019-01-22","No","No","No","Internal"]
[null,null,null,null,2641,"22_17/10/2019 5:26:28 AM","2019-01-31","Defect","Ship Staff","Ship Staff Insp.","STBD. HH crane hyd cylinder eye pin end plate holding bolt broken","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.5","Very High","","","Extracted Broken bolt and fixed new bolt","2019-02-15","","Completed","2019-02-05","No","No","No","Internal"]
[null,null,null,null,2642,"22_17/10/2019 5:31:53 AM","2019-01-31","Defect","Ship Staff","Ship Staff Insp.","ME starting air manifold, drain line exhaust gas leaking during engine running","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.1","Medium","","","Suspected unit 5 cyl starting air valve leaking. Starting air valve renewed and rectified leakage","2019-10-02","","Completed","2019-10-02","No","No","No","Internal"]
[null,null,null,null,2647,"22_17/10/2019 6:01:43 AM","2019-01-31","Defect","Ship Staff","Ship Staff Insp.","Flash back arrestors and pr regulations for gas welding to renew (as per new vetting requirements, 5 yrly renewal)","E/R - Aux. Mach.","Eng. / Strg. Comp.","Industry Issue","10.12","Very High","","","Spares received, fitted at Oxygen & acetylene bottles","2019-03-31","","Completed","2019-03-12","No","No","No","Internal"]
[null,null,null,null,2648,"22_17/10/2019 6:07:48 AM","2019-01-31","Defect","Ship Staff","Ship Staff Insp.","No. 1 FO purifier PCB defective in cold weather conditions , the PCB require warm heat, otherwise its function is satisfacory","E/R - Purifier","Eng. / Strg. Comp.","Equipment Related","10.12","Very High","","","New PCB recieved at Singapore and it is replaced, purifier now working satisfacory.","2019-03-16","DFAL180296","Completed","2019-03-14","No","No","No","Internal"]
[null,null,null,null,2713,"22_18/10/2019 8:22:56 AM","2019-01-31","Defect","Ship Staff","Ship Staff Insp.","Service air compressor oil filter base frame ( aluminium casing) to renew","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related","10.2","Low","","","Crack observed on the filter base threads, temporarily repaired and made new threads and used union of different size.","2019-05-15","DFAL190045","Completed","2019-04-23","No","No","No","Internal"]
[null,null,null,null,2725,"22_18/10/2019 8:50:00 AM","2019-01-31","Defect","Ship Staff","Ship Staff Insp.","Rotating beacon light for cargo oil tank high level alarm defective","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.14","Very High","","","New rotating beacon light received, same fitted in place, working satisfactorily","2019-05-31","","Completed","2019-05-31","No","No","No","Internal"]
[null,null,null,null,2729,"22_19/10/2019 12:49:17 AM","2019-01-31","Defect","Ship Staff","Ship Staff Insp.","No. 1 AC blower motor side pully to renew","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.2","Low","","","damaged pully replaced with new one.","2019-06-15","","Completed","2019-06-15","No","No","No","Internal"]
[null,null,null,null,2734,"22_19/10/2019 12:58:37 AM","2019-01-31","Defect","Ship Staff","Ship Staff Insp.","ME shaft earthing milli volt meter defective","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.2","Low","","","New volt meter fitted in place working satisfactorily.","2019-06-30","","Completed","2019-06-30","No","No","No","Internal"]
[null,null,null,null,2649,"22_17/10/2019 6:11:15 AM","2019-02-02","Defect","Ship Staff","Ship Staff Insp.","Emcy DG LO contamination due to cooler flange material erosion and jacket water leak from body cover, holed at multiple places","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.12","Very High","","","Jacket water cover and lube oil cooler renewed. Engine tried out no more leakages observed.","2019-03-28","DFAL190055","Completed","2019-03-11","No","No","No","Internal"]
[null,null,null,null,2651,"22_17/10/2019 6:16:04 AM","2019-02-03","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Elevator tracks and internals dirty","Elect. Mach. & Equip.","General Appearance","Equipment Related,External Factors","11.7","High","","","Elevator tracks and internals cleaned","2019-03-14","","Completed","2019-03-14","No","No","No","Internal"]
[null,null,null,null,2652,"22_17/10/2019 6:18:14 AM","2019-02-03","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ECR door handle needs repair/ replacement","Miscellaneous","General Appearance","Equipment Related","11.7","High","","","ECR door handle repaired","2019-03-14","","Completed","2019-03-14","No","No","No","Internal"]
[null,null,null,null,2653,"22_17/10/2019 6:21:17 AM","2019-02-03","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Gangway motors P&S oil stains around","Deck - Machinery","General Appearance","Equipment Related","11.7","High","","","Inspection of Filter & oiler unit carried out & rectified.","2019-03-15","","Completed","2019-03-15","No","No","No","Internal"]
[null,null,null,null,2654,"22_17/10/2019 6:24:44 AM","2019-02-03","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Accommodation random inspection- crew need to be reminded for better housekeeping","Accommodation","General Appearance","Behaviour Based","11.7","High","","","Random inspection carried out & ship staff reminded on better housekeeping","2019-03-15","","Completed","2019-03-17","No","No","No","Internal"]
[null,null,null,null,2670,"22_18/10/2019 12:44:33 AM","2019-02-03","Defect","Ship Staff","Ship Staff Insp.","IGS control air line filter leakage","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","8.22","Very High","","","IGS control air line filter renewed.","2019-03-31","","Completed","2019-03-13","No","No","No","Internal"]
[null,null,null,null,2718,"22_18/10/2019 8:37:47 AM","2019-02-05","Defect","Ship Staff","Ship Staff Insp.","Main air compressor no. 2 found leaking from Intercooler","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.2","Low","","","Intercooler gasket renewed, working satisfactory.","2019-05-15","","Completed","2019-05-02","No","No","No","Internal"]
[null,null,null,null,2735,"22_19/10/2019 1:00:02 AM","2019-02-15","Defect","Ship Staff","Ship Staff Insp.","Stbd. HH crane noise heard during lifting","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.5","Very High","","","Hyd. ram ( stbd.) lowering bearing renewed. working satisfactory.","2019-06-30","","Completed","2019-06-29","No","No","No","Internal"]
[null,null,null,null,9447,"22_1/7/2020 1:01:54 AM","2019-02-16","Defect","Ship Staff","Ship Staff Insp.","ONE OF THE BA SET LEAKING AT BA SET, BOTTLE HOSE CONNECTOR DURING ROUTINE DRILLS.","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","SPARE BA SET PUT IN USE, FAULTY BA SET REPLACED WITH SPARE BA SET AVAILABLE ONBOARD.","2019-02-17","","Completed","2019-02-17","No","No","No","Internal"]
[null,null,null,null,9967,"22_1/20/2020 2:24:33 PM","2019-02-16","Non Conformity","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ONE OF THE BA SET LEAKING AT BA SET, BOTTLE HOSE CONNECTOR DURING ROUTINE DRILLS.","Critical Equip.","Safety / LSA / FFA","Behaviour Based","","","","","SPARE BA SET PUT IN USE, FAULTY BA SET REPLACED WITH SPARE BA SET AVAILABLE ONBOARD.","2019-02-17","","Completed","2019-02-17","No","No","No","Internal"]
[null,null,null,null,9448,"22_1/7/2020 1:11:22 AM","2019-02-18","Non Conformity","Ship Staff","Ship Staff Insp.","LIFEBOATS NOT LOWERED IN WATER IN STIPULATED TIME AS REQUIRED.","LSA / FFA","Safety / LSA / FFA","External Factors","5.39","Very High","","","LIFEBOATS TO BE LOWERED IN WATER  AS & WHEN TIME/ WEATHER / VESSELS TRADING PATTERN ALLOWS BEFORE DUE DATE. SO THAT THE TIME FRAME OF 3 MONTHS WILL BE VALID TILL COMPLETION OF VOYAGE","2019-03-31","","Completed","2019-02-26","No","No","No","Internal"]
[null,null,null,null,9969,"22_1/20/2020 2:29:58 PM","2019-02-18","Non Conformity","Owner / Marine / Tech. Suptd.","Suptd. Insp.","LIFEBOATS NOT LOWERED IN WATER IN STIPULATED TIME AS REQUIRED.","Critical Equip.","Safety / LSA / FFA","External Factors","","","","","LIFEBOATS TO BE LOWERED IN WATER  AS & WHEN TIME/ WEATHER / VESSELS TRADING PATTERN ALLOWS BEFORE DUE DATE. SO THAT THE TIME FRAME OF 3 MONTHS WILL BE VALID TILL COMPLETION OF VOYAGE.","2019-02-19","","Completed","2019-02-26","No","No","No","Internal"]
[null,null,null,null,2643,"22_17/10/2019 5:34:20 AM","2019-02-25","Defect","Ship Staff","Ship Staff Insp.","NO. 2 WBP leaking at spool piece between strainer & pump casing","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.12","Medium","","","Temporary repairs carried out & job added in docking list for permanent repairs.","2019-03-31","","Completed","2019-02-28","No","No","No","Internal"]
[null,null,null,null,2650,"22_17/10/2019 6:13:26 AM","2019-02-27","Defect","Ship Staff","Ship Staff Insp.","ME OMD giving fault alarms randomly","E/R - Main Engine","","Equipment Related","10.21","Medium","","","Service engineer attended the job, checked the system and renewed the air pressure regulator","2019-10-03","","Completed","2019-03-09","No","No","No","Internal"]
[null,null,null,null,2655,"22_17/10/2019 6:29:48 AM","2019-03-03","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Officers mess windows to clean and cooler space to be covered neatly with wood","Accommodation","General Appearance","Behaviour Based","11.7","High","","","Windows cleaned & cooler space covered.","2019-03-23","","Completed","2019-03-20","No","No","No","Internal"]
[null,null,null,null,2672,"22_18/10/2019 12:48:13 AM","2019-03-03","Defect","Ship Staff","Ship Staff Insp.","Main engine jacket cooler sea water outlet section leakage from the flange","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.21","Medium","","","The leakage rectified by renewing the gasket.","2019-03-31","","Completed","2019-03-26","No","No","No","Internal"]
[null,null,null,null,2678,"22_18/10/2019 1:02:17 AM","2019-03-03","Defect","Ship Staff","Ship Staff Insp.","IGS and ejector pump no. 1 seal leaking and the performance poor.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","8.22","Very High","","","The pump overhauled, mouth ring renewed. The performance is satisfactory now.","2019-03-31","","Completed","2019-03-17","No","No","No","Internal"]
[null,null,null,null,2679,"22_18/10/2019 1:03:48 AM","2019-03-03","Defect","Ship Staff","Ship Staff Insp.","Fresh water generator distillate pump making abnormal noise.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.1","Medium","","","The distillate pump overhauled, mouth ring renewed. The performance is satisfactory now.","2019-03-31","","Completed","2019-03-16","No","No","No","Internal"]
[null,null,null,null,2680,"22_18/10/2019 1:05:17 AM","2019-03-03","Defect","Ship Staff","Ship Staff Insp.","Hydraulic power pack No. 2 motor flexible coupling worn out.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","9.15","Medium","","","The spider coupling renewed.","2019-03-31","","Completed","2019-03-15","No","No","No","Internal"]
[null,null,null,null,2684,"22_18/10/2019 1:40:34 AM","2019-03-03","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Wasted cable supports around accommodation to renew.","Elect. Mach. & Equip.","General Appearance","Equipment Related","11.7","High","","","Wasted cable supports around accommodation to renew at the earliest.","2019-03-31","","Completed","2019-03-22","No","No","No","Internal"]
[null,null,null,null,2686,"22_18/10/2019 1:44:37 AM","2019-03-03","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","CCR & ECR and various common places need to be aesthetically maintained.","Accommodation","General Appearance","Equipment Related","11.7","High","","","CCR & ECR to be aesthetically maintained.","2019-03-23","","Completed","2019-03-20","No","No","No","Internal"]
[null,null,null,null,2694,"22_18/10/2019 2:25:50 AM","2019-03-04","Defect","Ship Staff","Ship Staff Insp.","ME HFO line overflow piston valve leaking","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.9","Medium","","","Overflow piston valve overhauled, all the O rings renewed.","2019-04-15","","Completed","2019-04-05","No","No","No","Internal"]
[null,null,null,null,2695,"22_18/10/2019 2:27:23 AM","2019-03-04","Defect","Ship Staff","Ship Staff Insp.","AE Emergencty air operated valve between diesel oil line and HFO line leaking from gasket","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.2","Low","","","The leakage rectified by renewing the gasket.","2019-04-15","","Completed","2019-04-05","No","No","No","Internal"]
[null,null,null,null,2671,"22_18/10/2019 12:46:10 AM","2019-03-14","Defect","Ship Staff","Ship Staff Insp.","ECR AC sea water inlet pipe section wasted and leaking","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.2","Low","","","The pipe section fabricated and fitted.","2019-03-31","","Completed","2019-03-26","No","No","No","Internal"]
[null,null,null,null,2657,"22_17/10/2019 6:37:06 AM","2019-03-16","Defect","Ship Staff","Ship Staff Insp.","Oil leak observed from M4 mooring winc, found Regulator block leaking","Deck - Machinery","Mooring","Equipment Related","9.2","Very High","","","Regulator block overhauled & O-ring renewed","2019-04-30","","Completed","2019-03-19","No","No","No","Internal"]
[null,null,null,null,2673,"22_18/10/2019 12:50:46 AM","2019-03-16","Defect","Ship Staff","Ship Staff Insp.","ME air cooler no. 2 sea water inlet section leakage","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.2","Low","","","The inlet section leakage rectified by replacing the section with fabricated spare. The sacrificial section also renewed and all the gaskets renewed.","2019-03-31","","Completed","2019-03-26","No","No","No","Internal"]
[null,null,null,null,2674,"22_18/10/2019 12:54:13 AM","2019-03-16","Defect","Ship Staff","Ship Staff Insp.","Main engine Air cooler No. 1 sea water inlet and outlet section leakage ","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.2","Low","","","The inlet section flange side welding totally wasted, the same build up by welding. The inlet side sacrificial section renewed. The outlet section replaceed with fabricated spare.","2019-03-31","","Completed","2019-03-26","No","No","No","Internal"]
[null,null,null,null,2731,"22_19/10/2019 12:53:05 AM","2019-03-16","Defect","Ship Staff","Ship Staff Insp.","Oil leak observed from port windlass winch","Deck - Mooring Machinery","Mooring","Equipment Related","9.16","High","","","New hydraulic motor fitted in place. Tried out working satisfactorily.","2019-06-15","","Completed","2019-06-15","No","No","No","Internal"]
[null,null,null,null,2668,"22_18/10/2019 12:41:07 AM","2019-03-18","Defect","Ship Staff","Ship Staff Insp.","AE jacket cooler no. 1 sea water inlet section to renew as leakage is their from the flange","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.2","Low","","","The inlet section replaced with fabricated one.","2019-03-31","","Completed","2019-03-27","No","No","No","Internal"]
[null,null,null,null,2689,"22_18/10/2019 1:49:46 AM","2019-03-18","Defect","Ship Staff","Ship Staff Insp.","Light base around accomodation area wasted","Elect. Mach. & Equip.","General Appearance","Equipment Related","11.7","High","","","New base fabricated.","2019-04-30","","Completed","2019-04-05","No","No","No","Internal"]
[null,null,null,null,2665,"22_2019-10-17 07:18:04.999","2019-03-19","Defect","Ship Staff","Ship Staff Insp.","Main Engine unit No. 3 aft high  pressure pipe leakage from pump side.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.2","Low","","","The leakage rectified by overhauling the high pressure pipe","2019-03-31","","Completed","2019-04-26","No","No","No","Internal"]
[null,null,null,null,2675,"22_18/10/2019 12:56:04 AM","2019-03-19","Defect","Ship Staff","Ship Staff Insp.","Main engine HFO Autobackwash filter inlet and outlet valves not holding.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.2","Low","","","The inlet and outlet valves renewed.","2019-03-31","","Completed","2019-03-24","No","No","No","Internal"]
[null,null,null,null,2676,"22_18/10/2019 12:58:19 AM","2019-03-20","Defect","Ship Staff","Ship Staff Insp.","Aux boiler no. 1 steam return valve from economiser leaking from bonnet.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.9","Medium","","","The valve overhauled, gland packing and bonnet gasket renewed.","2019-03-31","","Completed","2019-03-25","No","No","No","Internal"]
[null,null,null,null,2677,"22_18/10/2019 1:00:02 AM","2019-03-20","Defect","Ship Staff","Ship Staff Insp.","ME lube oil cooler sea water inlet section leaking","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.7","Medium","","","The sea water inlet section found totally wasted at the flange, the same build up by welding. The inlet valve also renewed.","2019-03-31","","Completed","2019-03-30","No","No","No","Internal"]
[null,null,null,null,2683,"22_18/10/2019 1:38:59 AM","2019-03-20","Defect","Ship Staff","Ship Staff Insp.","Rudder carrier oil tank leakage.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.16","Very High","","","The gauge glass both side packing renewed and the supply line leakage rectified.","2019-03-31","","Completed","2019-03-29","No","No","No","Internal"]
[null,null,null,null,2666,"22_2019-10-17 07:20:25.000","2019-03-21","Defect","Ship Staff","Ship Staff Insp.","Spring air line have a pin hole to rectify","Deck - Mooring Machinery","","Equipment Related","9.5","High","","","The leakage rectified by renewing the section","2019-03-31","","Completed","2019-03-25","No","No","No","Internal"]
[null,null,null,null,2663,"22_17/10/2019 6:55:56 AM","2019-03-22","Defect","Ship Staff","Ship Staff Insp.","Main engine Unit no. 3, 6 and 7 exhaust gas leakage from bellow","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.12","Very High","","","The leakage rectified by realigning the bellows","2019-03-31","","Completed","2019-03-28","No","No","No","Internal"]
[null,null,null,null,2664,"22_17/10/2019 6:58:07 AM","2019-03-22","Defect","Ship Staff","Ship Staff Insp.","Main engine unit No. 4 and 7 exhaust valve hydraulic line leakage","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.13","Very High","","","The leakage rectified by removing the O-rings","2019-03-31","","Completed","2019-03-23","No","No","No","Internal"]
[null,null,null,null,2687,"22_18/10/2019 1:46:09 AM","2019-03-24","Defect","Ship Staff","Ship Staff Insp.","AE No. 3 LT water outlet valve bridge found broken","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.2","Low","","","The valve renewed.","2019-03-31","","Completed","2019-03-27","No","No","No","Internal"]
[null,null,null,null,2681,"22_18/10/2019 1:07:44 AM","2019-03-25","Defect","Ship Staff","Ship Staff Insp.","E/R blower flaps not colsing properly","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.2","Low","","","All the flaps greasing carried out and at the sealing surface fire resistant packing placed. Now the doors are closing positively.","2019-03-31","","Completed","2019-03-30","No","No","No","Internal"]
[null,null,null,null,2682,"22_18/10/2019 1:09:28 AM","2019-03-25","Defect","Ship Staff","Ship Staff Insp.","E/R funnel hatch covers not sealing positively.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.11","Medium","","","The funnel hatch covers packings renewed and additional fire resistant packing fitted in such a way that the doors are closing positively now.","2019-03-31","","Completed","2019-03-30","No","No","No","Internal"]
[null,null,null,null,2688,"22_18/10/2019 1:48:15 AM","2019-03-26","Defect","Ship Staff","Ship Staff Insp.","AC condenser sea water outlet pressure gauge, Ref condenser sea water outlet ressure gauge. Main engine unit no. 6 jacket cooluing water outlet temperature gauge, AE No. 3 Fuel oil inlet temperature gauge defective","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.2","Low","","","All defective pressure and temperature gauges renewed.","2019-03-31","","Completed","2019-03-30","No","No","No","Internal"]
[null,null,null,null,2690,"22_18/10/2019 1:52:32 AM","2019-03-29","Defect","Ship Staff","Ship Staff Insp.","ME fuel oil supply pump no. 1 considerable leakage is there from gland.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.8","Medium","","","ME supply pump no. 1 overhauled, bearing metal and gland packing renewed.","2019-04-15","","Completed","2019-04-01","No","No","No","Internal"]
[null,null,null,null,2691,"22_18/10/2019 2:07:11 AM","2019-03-29","Defect","Ship Staff","Ship Staff Insp.","ME fuel oil circulating pump no. 2 considerable leakage is there from gland.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.17","Very High","","","ME circulating pump no. 2 overhauled, bearing metal and gland packing renewed.","2019-04-15","","Completed","2019-04-01","No","No","No","Internal"]
[null,null,null,null,2685,"22_18/10/2019 1:42:24 AM","2019-04-03","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Both cargo manifold tray gratings corroded.","Miscellaneous","General Appearance","Equipment Related","11.7","High","","","Derusting & painting to be carried out for manifold drip tray gratings","2019-04-30","","Completed","2019-04-23","No","No","No","Internal"]
[null,null,null,null,2696,"22_18/10/2019 2:29:37 AM","2019-04-03","Defect","Ship Staff","Ship Staff Insp.","ME HFO inlet to heater no. 1 valve gland packing renewed.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.2","Low","","","The valve gland packing renewed.","2019-04-15","","Completed","2019-05-04","No","No","No","Internal"]
[null,null,null,null,2714,"22_18/10/2019 8:24:30 AM","2019-04-03","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Gantry crane poor cosmetics. ","Deck - Machinery","General Appearance","Equipment Related","11.7","High","","","Derusting & painting of the gantry crane track completed.","2019-04-30","","Completed","2019-04-30","No","No","No","Internal"]
[null,null,null,null,2736,"22_19/10/2019 1:01:47 AM","2019-04-03","Defect","Ship Staff","Ship Staff Insp.","In Musasino tank radar system, Slop S COT, shows reading as 16% filled, where as the tank is empty.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.12","Medium","","","Job being attended by Musasino in DD, work in progress.","2019-04-07","","Completed","2019-07-04","No","No","No","Internal"]
[null,null,null,null,2697,"22_18/10/2019 2:32:03 AM","2019-04-04","Defect","Ship Staff","Ship Staff Insp.","Port Hose handling crane Hyd. metal pipes for boom/heave (up and down) ruptured and oil was leaking heavily.","Deck - Machinery","Cargo / Ballast Systems","Equipment Related","8.5","Very High","","","5 piece of metal pipes replaced with new spares available onboard.","2019-04-30","","Completed","2019-04-18","No","No","No","Internal"]
[null,null,null,null,2719,"22_18/10/2019 8:39:05 AM","2019-04-05","Defect","Ship Staff","Ship Staff Insp.","Boiler fuel oil burning pump no. 2 found leaking from mechanical seal","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.9","Medium","","","Complete pump replaced with new one.","2019-05-15","","Completed","2019-05-06","No","No","No","Internal"]
[null,null,null,null,2720,"22_18/10/2019 8:40:23 AM","2019-04-05","Defect","Ship Staff","Ship Staff Insp.","2P bunker tank steam inlet valve found leaking ","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.8","Medium","","","Valve bonnet gasket renewed.","2019-05-15","","Completed","2019-05-06","No","No","No","Internal"]
[null,null,null,null,2704,"22_18/10/2019 3:25:01 AM","2019-04-16","Defect","Ship Staff","Ship Staff Insp.","MSB room AC Sea water inlet section leaking","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.2","Low","","","The section fabricated and fitted","2019-04-30","","Completed","2019-04-16","No","No","No","Internal"]
[null,null,null,null,2705,"22_18/10/2019 3:27:10 AM","2019-04-16","Defect","Ship Staff","Ship Staff Insp.","Both EGB soot blower motor have some vibration and abnormal noise","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.2","Low","","","Both motors overhauled","2019-04-30","","Completed","2019-04-16","No","No","No","Internal"]
[null,null,null,null,2706,"22_18/10/2019 3:43:00 AM","2019-04-16","Defect","Ship Staff","Ship Staff Insp.","Drain Scupper section from lube oil cooler area to stbd. bilge well fully rusted","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.2","Low","","","Section fabricated and fitted","2019-04-30","","Completed","2019-04-17","No","No","No","Internal"]
[null,null,null,null,2698,"22_18/10/2019 2:34:24 AM","2019-04-17","Defect","Ship Staff","Ship Staff Insp.","Hydraulic return line for Port HHC found to be leaking","Deck - Machinery","Cargo / Ballast Systems","Equipment Related","8.5","Very High","","","Section of leaking pipe dismantled, repaired & put back in place. Tried out the crane after installation. No leaks observed.","2019-04-30","","Completed","2019-04-18","No","No","No","Internal"]
[null,null,null,null,2699,"22_18/10/2019 2:36:04 AM","2019-04-17","Defect","Ship Staff","Ship Staff Insp.","Observed a twist  in Port & Stbd anchor cable","Deck - Mooring Machinery","Mooring","Equipment Related","8.5","Very High","","","Twist removed from P & S anchor cable","2019-04-30","","Completed","2019-04-24","No","No","No","Internal"]
[null,null,null,null,2707,"22_18/10/2019 3:47:06 AM","2019-04-17","Defect","Ship Staff","Ship Staff Insp.","Steam tracing line for HFO found leaking","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.2","Low","","","Leakage rectified","2019-04-17","","Completed","2019-04-30","No","No","No","Internal"]
[null,null,null,null,2708,"22_18/10/2019 8:14:16 AM","2019-04-17","Defect","Ship Staff","Ship Staff Insp.","HFO circulating pump no. 1 leaking from gland packing","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.8","Medium","","","Leakage rectified by renewing the packing","2019-04-30","","Completed","2019-04-20","No","No","No","Internal"]
[null,null,null,null,2715,"22_18/10/2019 8:25:56 AM","2019-04-18","Defect","Ship Staff","Ship Staff Insp.","Found 7 numbers of foam hydrants leaking","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.38","High","","","Leak rectified for all 7 foam hydrants.","2019-04-30","","Completed","2019-04-30","No","No","No","Internal"]
[null,null,null,null,2701,"22_18/10/2019 2:40:05 AM","2019-04-19","Defect","Ship Staff","Ship Staff Insp.","Main steam inlet valve for heating coils on deck found leaking.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.15","High","","","Gasket to be removed.","2019-04-30","","Completed","2019-04-26","No","No","No","Internal"]
[null,null,null,null,2702,"22_18/10/2019 3:20:56 AM","2019-04-19","Defect","Ship Staff","Ship Staff Insp.","Mooring winch M4 interconnection line between two hydraulic motor found leaking.","Deck - Mooring Machinery","Mooring","Equipment Related","9.16","High","","","This line section removed from place and both side O-rings renewed.","2019-04-30","","Completed","2019-04-26","No","No","No","Internal"]
[null,null,null,null,2703,"22_18/10/2019 3:23:18 AM","2019-04-19","Defect","Ship Staff","Ship Staff Insp.","All three AE lube oil priming pump have some abnormal noise and vibration","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.2","Low","","","All three motors overhauled, now working satisfactory.","2019-04-30","","Completed","2019-04-20","No","No","No","Internal"]
[null,null,null,null,2712,"22_18/10/2019 8:20:52 AM","2019-04-19","Defect","Ship Staff","Ship Staff Insp.","AE diesel oil flushing pump leakage from pump cover","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.2","Low","","","The pump overhauled","2019-04-30","","Completed","2019-04-24","No","No","No","Internal"]
[null,null,null,null,2709,"22_18/10/2019 8:15:57 AM","2019-04-20","Defect","Ship Staff","Ship Staff Insp.","All three AE pressure gauge panel not secured properly","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.2","Low","","","Pressure gauge panel secured firmly","2019-04-30","","Completed","2019-04-21","No","No","No","Internal"]
[null,null,null,null,2700,"22_18/10/2019 2:37:51 AM","2019-04-21","Defect","Ship Staff","Ship Staff Insp.","2 chairs hand rest found broken in Officer's Mess room","Accommodation","General Appearance","Equipment Related","11.7","High","","","Hand rest repaired for both the chairs & chairs put in use.","2019-04-28","","Completed","2019-04-24","No","No","No","Internal"]
[null,null,null,null,2710,"22_18/10/2019 8:17:30 AM","2019-04-23","Defect","Ship Staff","Ship Staff Insp.","AE no. 2 sump oil low level alarm found inoperational.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.2","Low","","","The sensor cleaned and sensor chamber cleared of sludge. The alarm is operating now.","2019-04-30","","Completed","2019-04-23","No","No","No","Internal"]
[null,null,null,null,2711,"22_18/10/2019 8:19:17 AM","2019-04-23","Defect","Ship Staff","Ship Staff Insp.","EGE feed pump no. 2 suction valve leakage from valve bonnet","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.2","Low","","","Leakage rectified by renewing the packing","2019-04-30","","Completed","2019-04-24","No","No","No","Internal"]
[null,null,null,null,2730,"22_19/10/2019 12:51:23 AM","2019-05-02","Defect","Ship Staff","Ship Staff Insp.","AMS-field station - F, CPU module defective , due to this all DG alarms went offline and could not be monitored from AMS panel","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.2","Low","","","New plc card received, same fitted in place. tried out, working satisfactorily.","2019-06-15","","Completed","2019-06-15","No","No","No","Internal"]
[null,null,null,null,2726,"22_18/10/2019 8:53:47 AM","2019-05-03","Defect","Ship Staff","Ship Staff Insp.","4P COT Temperature reading incorrect in Musasino tank radar system.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.12","Medium","","","New sensor recieved, temperature sensor element renewed. Now working satisfactorily.","2019-05-31","","Completed","2019-05-24","No","No","No","Internal"]
[null,null,null,null,2727,"22_19/10/2019 12:02:52 AM","2019-05-03","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Gantry crane cable drum winding mechanism to repair","Deck - Machinery","General Appearance","Equipment Related","11.7","High","","","Cable drum winding mechanism overhauling carried out found working satisfactorily","2019-06-15","","Completed","2019-05-26","No","No","No","Internal"]
[null,null,null,null,2728,"22_19/10/2019 12:47:57 AM","2019-05-03","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Several lagging in engine room plan to renew during scrubber installation time","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.2","Low","","","Several lagging in engine room renewed.","2019-06-15","","Completed","2019-05-29","No","No","No","Internal"]
[null,null,null,null,2716,"22_18/10/2019 8:28:00 AM","2019-05-04","Defect","Ship Staff","Ship Staff Insp.","Cargo Tank 2P overfill alarm not reseting due to fault with PAXD-Module card","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.12","Medium","","","Module card renewed, working satisfacorily","2019-05-15","DFAL190121","Completed","2019-05-12","No","No","No","Internal"]
[null,null,null,null,2717,"22_18/10/2019 8:30:04 AM","2019-05-04","Defect","Ship Staff","Ship Staff Insp.","Slop P fault with overfill alarm due to fault with PAXD-Module card","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.12","Medium","","","Module card renewed, working satisfactorily","2019-05-15","","Completed","2019-05-12","No","No","No","Internal"]
[null,null,null,null,2721,"22_18/10/2019 8:41:42 AM","2019-05-05","Defect","Ship Staff","Ship Staff Insp.","COPT gland steam line found leaking as it developed cracks.","Cargo Mach.","Eng. / Strg. Comp.","Equipment Related","8.8","Medium","","","The crack repaired by welding.","2019-05-15","","Completed","2019-05-06","No","No","No","Internal"]
[null,null,null,null,2723,"22_18/10/2019 8:46:12 AM","2019-05-05","Defect","Ship Staff","Ship Staff Insp.","AE #1 fuel oil line pulse damper leaking","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.2","Low","","","The pulse damper assembly removed from place, both side O-rings renewed and fitted back. Working satisfactorily","2019-05-15","","Completed","2019-05-11","No","No","No","Internal"]
[null,null,null,null,2724,"22_18/10/2019 8:47:46 AM","2019-05-05","Defect","Ship Staff","Ship Staff Insp.","ME shock absorber unit #6 found leaking","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.2","Low","","","Unit No. 6 shock absorber overhauled, sealing and wear rings renewed.","2019-05-15","","Completed","2019-05-14","No","No","No","Internal"]
[null,null,null,null,9453,"22_1/7/2020 1:32:56 AM","2019-05-10","Non Conformity","Ship Staff","Ship Staff Insp.","Form 05.05.00.001.01  KPI  SHIP REPORT for Month Of September 2019, was not renamed and sent. ","Miscellaneous","ISM Related","Inappropriate Procedure","","","","","Officer to use new form ecah time and same to be verified by another officer or senior officer for correctness, to eliminate errors arising due to Complacency","2019-11-21","","Completed","2019-11-18","No","No","No","Internal"]
[null,null,null,null,9975,"22_1/20/2020 2:42:00 PM","2019-05-10","Non Conformity","Ship Staff","Suptd. Insp.","Form 05.05.00.001.01  KPI  SHIP REPORT for Month Of September 2019, was not renamed and sent. ","Documentation","Cert. & Docu.","Behaviour Based","","","","","Officer to use new form ecah time and same to be verified by another officer or senior officer for correctness, to eliminate errors arising due to Complacency","2019-01-11","","Completed","2019-10-30","No","No","No","Internal"]
[null,null,null,null,2733,"22_19/10/2019 12:56:06 AM","2019-05-13","Defect","Ship Staff","Ship Staff Insp.","ME cylinder head unit #1 exhaust gas outlet temerature gauge faulty ","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.2","Low","","","New pyrometer received. Same fitted in place.","2019-06-15","","Completed","2019-06-15","No","No","No","Internal"]
[null,null,null,null,9965,"22_1/20/2020 2:19:36 PM","2019-05-21","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","While Navigating in the Channel or Vessel at berth, Transit bearing used to check the accuracy of compass error enteries were missing in Deck log book.","Navigation - Others","Navigation","Human Error","","","","","Discussed with all navigating officer’s & emphasized on to follow the Master standing order and company’s procedure’s correctly at all times.","2019-05-23","","Completed","2019-05-23","No","No","No","Internal"]
[null,null,null,null,2669,"22_18/10/2019 12:43:06 AM","2019-06-03","Defect","Ship Staff","Ship Staff Insp.","No. 2 steering gear servo pump, oil leakage observed from tell tale hole, seal to renew.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.39","High","","","Servo pump overhauled and the oil seal renewed","2019-08-04","","Completed","2019-08-07","No","No","No","Internal"]
[null,null,null,null,9449,"22_1/7/2020 1:15:11 AM","2019-06-04","Non Conformity","Ship Staff","Ship Staff Insp.","AC duct fresh air intake flaps unable to operate from outside operating lever. The duct outside portion was fully corroded and holed. When this duct section was removed we found the flaps were totally wasted.","Elect. Mach. & Equip.","Structural Condn. / WT integrity ","Equipment Related","","","","","The duct section along with flap removed from place, brought to Engine room workshop. New flaps fabricated and also the corroded section of the duct repaired and this section fitted back in place. The flap operation tried out, found working satisfactorily","2019-04-15","","Completed","2019-04-10","No","No","No","Internal"]
[null,null,null,null,9970,"22_1/20/2020 2:32:19 PM","2019-06-04","Non Conformity","Owner / Marine / Tech. Suptd.","Suptd. Insp.","AC duct fresh air intake flaps unable to operate from outside operating lever. The duct outside portion was fully corroded and holed. When this duct section was removed we found the flaps were totally wasted.","Miscellaneous","Emgcy. Systems","Equipment Related","","","","","The duct section along with flap removed from place, brought to Engine room workshop. New flaps fabricated and also the corroded section of the duct repaired and this section fitted back in place. The flap operation tried out, found working satisfactorily","2019-04-30","","Completed","2019-04-10","No","No","No","Internal"]
[null,null,null,null,2761,"22_19/10/2019 2:21:14 AM","2019-06-07","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Chemical Locker to be arranged","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.2","Low","","","Chemical locker arranged as per alkaline/acidic properties","2019-07-31","","Completed","2019-08-21","No","No","No","Internal"]
[null,null,null,null,8683,"22_Fri Dec 20 2019 23:49:59 GMT+0000 (Coordinated Universal Time)","2019-06-07","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Conduit line U-clamps to be derusted / painted and renewed where required.","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.7","High","","","Conduit lines U-CLAMPS renewed","2020-05-05","","Completed","2020-04-05","No","No","No","Internal","work in progress: Revised completion date; kindly complete prior to that.\nPart  completed,"]
[null,null,null,null,2656,"22_17/10/2019 6:34:37 AM","2019-07-03","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Bridge window shades to repair","Accommodation","General Appearance","Equipment Related","11.7","High","","","To overhaul the bridge window shades","2019-10-05","","Completed","2019-10-21","No","No","No","Internal"]
[null,null,null,null,2737,"22_19/10/2019 1:03:27 AM","2019-07-04","Defect","Ship Staff","Ship Staff Insp.","Aux. boiler feed pump No. 1 bearing housing worn out.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.9","Medium","","","received spare bearing housing fitted on place. Pump tried out working satisfactorily.","2019-07-15","","Completed","2019-07-15","No","No","No","Internal"]
[null,null,null,null,2738,"22_19/10/2019 1:14:01 AM","2019-07-06","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Grating near break of accomodation to derust and paint.","Miscellaneous","General Appearance","Equipment Related","11.7","High","","","Renewed parts of grating and painted","2019-08-11","","Completed","2019-08-20","No","No","No","Internal"]
[null,null,null,null,2744,"22_19/10/2019 1:31:00 AM","2019-07-06","Defect","Ship Staff","Ship Staff Insp.","Mooring winch hydraulic lines bar supports to be renewed at 5 locations","Deck - Pipe / Fittings","General Appearance","Equipment Related","9.1","Low","","","New supports fabricated and renewed","2019-08-31","","Completed","2019-08-01","No","No","No","Internal"]
[null,null,null,null,2747,"22_19/10/2019 1:35:16 AM","2019-07-06","Defect","Ship Staff","Ship Staff Insp.","Mooring fairleads grooving to be filled up total 20 nos.","Miscellaneous","General Appearance","Equipment Related","11.7","High","","","Completed","2019-08-31","","Completed","2019-08-01","No","No","No","Internal"]
[null,null,null,null,2740,"22_19/10/2019 1:25:19 AM","2019-07-07","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Working platform next to Main IG V/v to be renewed","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.7","High","","","New platform fabricated and renewed","2019-11-08","","Completed","2019-07-28","No","No","No","Internal"]
[null,null,null,null,2742,"22_19/10/2019 1:27:56 AM","2019-07-07","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Paint locker to be arranged","Miscellaneous","General Appearance","Behaviour Based","11.7","High","","","Completed.","2019-11-08","","Completed","2019-07-21","No","No","No","Internal"]
[null,null,null,null,2765,"22_2019-10-20 03:15:34.000","2019-07-08","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","CO2 room exhaust fan frame to be renewed","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.7","High","","","Frame renewed by fabrication","2019-08-11","","Completed","2019-06-09","No","No","No","Internal"]
[null,null,null,null,9966,"22_1/20/2020 2:22:15 PM","2019-07-10","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Echo Sounder Running Scale was missing in Deck log Book, Instructed To OOW to Log down in the Log Book. ","Navigation - Echo Sounder / Speed Log","Navigation","Human Error","","","","","All OOW informed about importance of monitering scale.","2019-07-11","","Completed","2019-10-28","No","No","No","Internal"]
[null,null,null,null,8680,"22_Fri Dec 20 2019 23:42:00 GMT+0000 (Coordinated Universal Time)","2019-07-15","Defect","Ship Staff","Ship Staff Insp.","All three AVRs fitted on MSB are different type and having problem for running No.1 and No.3 DGs in parallel","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.1","Medium","","","Service technicians attended in singapore and renewed all three AVRs(AVC 63-12B) with Transformer,tuning was carried out, operation is satisfactory.","2019-10-30","","Completed","2019-10-24","No","No","No","Internal","job attended and closed out in Singapore / refer to serv reports and close out"]
[null,null,null,null,2658,"22_17/10/2019 6:39:11 AM","2019-08-03","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","COW branch valve found very hard to open / shut","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.11","Medium","","","All COW machine valves lubricated & freed up","2019-08-04","","Completed","2019-08-20","No","No","No","Internal"]
[null,null,null,null,2659,"22_17/10/2019 6:43:07 AM","2019-08-03","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Funnel casing cleaning and painting","Miscellaneous","General Appearance","External Factors","11.7","High","","","Funnel casing cleaned / Derusted as required and painted","2019-08-06","","Completed","2019-08-25","No","No","No","Internal"]
[null,null,null,null,2660,"22_17/10/2019 6:49:29 AM","2019-08-03","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","IG Branch valves found very hard to open / shut","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.3","Very High","","","Degreasing / lubrication of worm gear actuator carried out for manifold valves & valves freed up","2019-08-04","","Completed","2019-08-27","No","No","No","Internal"]
[null,null,null,null,2661,"22_17/10/2019 6:51:34 AM","2019-08-03","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Manifold valves P&S found very hard to open/ shut","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.11","Medium","","","Degreasing & lubrication of worm gear actuator carried out for manifold valves & valves freed up.","2019-08-04","","Completed","2019-08-31","No","No","No","Internal"]
[null,null,null,null,9978,"22_1/20/2020 2:51:03 PM","2019-08-05","Non Conformity","FSC Inspector","PSC Inspection","Lifeboat Painter of Stbd Lifeboat Not Correctly Connected To Quick Release device","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","Life saving appliances","","Lifeboat Painter was correctly connected to quick release mechanism, and same was tried for its operation","2019-08-05","","Completed","2019-05-08","No","No","No","External"]
[null,null,null,null,9979,"22_1/20/2020 2:52:54 PM","2019-08-05","Non Conformity","FSC Inspector","PSC Inspection","Wheelhouse door not kept gastight and vapourtight when closed","Navigation - Others","General Appearance","Equipment Related","","","Water/Weathertight condition","","The rubber packing for wheelhouse doors were immediately adjusted and the doors were tested to be air/gas tight ,as noted by the class inspector","2019-08-05","","Completed","2019-05-08","No","No","No","External"]
[null,null,null,null,9980,"22_1/20/2020 2:54:38 PM","2019-08-05","Non Conformity","FSC Inspector","PSC Inspection","The handle of axe for fireman outfit was not provided with high voltage insulation completely.","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","Life saving appliances","","New requisition was made of fully insulated axe at port and same was supplied at the same port.","2019-08-05","","Completed","2019-05-08","No","No","No","External"]
[null,null,null,null,9981,"22_1/20/2020 2:56:50 PM","2019-08-05","Non Conformity","FSC Inspector","PSC Inspection","One cable hole penetrating the bulkhead of electrical equipment room not sealed.","Elect. Mach. & Equip.","Structural Condn. / WT integrity ","Equipment Related","","","Structural condition","","Immediately the bulkhead cable penetrating hole was sealed with sealing compound.","2019-08-05","","Completed","2019-05-08","No","No","No","External"]
[null,null,null,null,9982,"22_1/20/2020 2:58:45 PM","2019-08-05","Non Conformity","FSC Inspector","PSC Inspection","The corridors as means of escape on e-deck in accomodation space lack of handrail.","Accommodation","Emgcy. Systems","Equipment Related","","","Emergency Systems","","New Handrailing was fabricated through class approval in Yiulian Shipyard , China","2019-08-07","","Completed","2019-06-07","No","No","No","External"]
[null,null,null,null,2739,"22_19/10/2019 1:16:06 AM","2019-08-07","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","DO bunkering line to derust and paint.","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.7","High","","","Completed","2019-11-08","","Completed","2019-08-18","No","No","No","Internal"]
[null,null,null,null,2741,"22_19/10/2019 1:26:26 AM","2019-08-07","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Derusting and Painting of Mooring winches","Deck - Mooring Machinery","General Appearance","Equipment Related","9.11","Medium","","","Completed","2019-11-08","","Completed","2019-08-22","No","No","No","Internal"]
[null,null,null,null,7331,"22_Mon Dec 16 2019 07:28:22 GMT+0000 (Coordinated Universal Time)","2019-08-09","Defect","Ship Staff","Ship Staff Insp.","SVDR REMOTE ALARM UNIT GIVING FAULTY ALARM. AS PER SERVICE TECHNICIAN ADVICE SAME NEEDS TO BE REPLACED WITH A NEW ONE.","Navigation - VDR / BNWAS","Navigation","Equipment Related","4.11","Medium","","","NEW UNIT RECIEVED. UNIT INSTALLED. SYSTEM CONFIGURED.","2020-04-25","","Completed","2020-04-25","No","No","No","Internal","upgrade completed last call Singapore..............kindly close out"]
[null,null,null,null,9452,"22_1/7/2020 1:25:32 AM","2019-08-09","Non Conformity","Ship Staff","Ship Staff Insp.","ALCOHOL ISSUE PROCEDURE NOT FOLLOWED ONBOARD, 08.22.01.00.01 STATES 2 OPEN CANS OF BEER TO BE ISSUED TO INDIVIDUALS, INSTEAD BEER CANS WERE ISSUED TO CREW MEMBERS WITHOUT OPENING.","Miscellaneous","ISM Related","Inappropriate Procedure","","","","","\"08.22.00.00.01 COMPANY RULES FOR ALCOHOL AND DRUGS\" were read and understood by all.","2019-10-09","","Completed","2019-09-09","No","No","No","Internal"]
[null,null,null,null,9974,"22_1/20/2020 2:38:48 PM","2019-08-09","Observation","Ship Staff","Suptd. Insp.","ALCOHOL ISSUE PROCEDURE NOT FOLLOWED ONBOARD, 08.22.01.00.01 STATES 2 OPEN CANS OF BEER TO BE ISSUED TO INDIVIDUALS, INSTEAD BEER CANS WERE ISSUED TO CREW MEMBERS WITHOUT OPENING.","Miscellaneous","Crew Management","Behaviour Based","","","","","Procedure for issuing beer cans without opening was immediately stopped and \"08.22.00.00.01 COMPANY RULES FOR ALCOHOL AND DRUGS\" were strictly complied with.","2019-09-09","","Completed","2019-09-09","No","No","No","Internal"]
[null,null,null,null,2743,"22_19/10/2019 1:29:18 AM","2019-08-14","Defect","Ship Staff","Ship Staff Insp.","Pump room davit lubricator broken","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.5","Very High","","","Renewed.","2019-08-22","","Completed","2019-08-14","No","No","No","Internal"]
[null,null,null,null,2745,"22_19/10/2019 1:32:47 AM","2019-08-16","Defect","Ship Staff","Ship Staff Insp.","4S PV Valve pressure side leaking","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.19","High","","","Opened and lapping done , satisfactory now","2019-08-22","","Completed","2019-08-16","No","No","No","Internal"]
[null,null,null,null,2746,"22_19/10/2019 1:34:09 AM","2019-08-16","Defect","Ship Staff","Ship Staff Insp.","1C PV Valve vaccum side leaking","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.19","High","","","Opened and lapping done , satisfactory now","2019-08-22","","Completed","2019-08-17","No","No","No","Internal"]
[null,null,null,null,2624,"22_2019-10-12 06:23:19.000","2019-08-17","Defect","Ship Staff","Ship Staff Insp.","Port side Hose handling crane limit switch leaking.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.5","Very High","","","Opened and cleaned the limit switch and o-Ring renewed, refitted and crane tried out no leak. Replaced with New One.","2019-12-25","DFAL190264","Completed","2019-12-17","No","No","No","Internal","high priority job, followup for spares and close out on receipt of spares"]
[null,null,null,null,7333,"22_Sat Oct 12 2019 06:23:19 GMT+0000 (Coordinated Universal Time)","2019-08-17","Breakdown","Ship Staff","Ship Staff Insp.","Port side Hose handling crane limit switch leaking.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.5","Very High","","","Opened and cleaned the limit switch and o-Ring renewed, refitted and crane tried out no leak, Load test done after repair, Recieved a new Limit switch. fitted & tested","2019-12-25","DFAL190264","Completed","2019-10-31","No","No","No","Internal"]
[null,null,null,null,2773,"22_20/10/2019 5:25:14 PM","2019-08-22","Defect","Ship Staff","Ship Staff Insp.","Valve indicator for COV 834 & COV 914 flickers when operated intermittent","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.11","Medium","","","COV 934indicator limits were adjusted and working satisfactory. COV 914 position indicator unit renewed.","2019-09-20","","Completed","2019-01-10","No","No","No","Internal"]
[null,null,null,null,2774,"22_20/10/2019 5:27:03 PM","2019-08-22","Defect","Ship Staff","Ship Staff Insp.","One hydraulic box hinge got broken","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.1","Very High","","","Completed.","2019-05-10","","Completed","2019-04-10","No","No","No","Internal"]
[null,null,null,null,9451,"22_1/7/2020 1:22:32 AM","2019-08-23","Non Conformity","FSC Inspector","OM Insp. (Eg. SIRE / CDI etc.)","SOPEP Manual not signed by Chief Engineer and ETO for read and understood.","Miscellaneous","ISM Related","Human Error","5.36","Low","","","Manual was read and understood by both CHENG & ETO and signed on 29th Aug 2019.","2019-08-29","","Completed","2019-08-29","No","No","No","External"]
[null,null,null,null,9973,"22_1/20/2020 2:36:08 PM","2019-08-23","Non Conformity","Owner / Marine / Tech. Suptd.","Suptd. Insp.","SOPEP Manual not signed by Chief Engineer and ETO for read and understood.","Documentation","Crew Management","Behaviour Based","","","","","Manual was read and understood by both CHENG & ETO and signed on 29th Aug 2019.","2019-08-31","","Completed","2019-08-29","No","No","No","Internal"]
[null,null,null,null,2763,"22_2019-10-19 02:27:15.000","2019-08-25","Defect","Ship Staff","Ship Staff Insp.","During discharging at Map ta Phut on 2nd  day of discharge Cargo system Bulkheadmaster v/v COV831 could not be opened when restarting the cargo discharge after a shore stoppage.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.11","Medium","","","operated manually activating the solenoid, solenoid coil on open side require renewal","2019-09-10","","Completed","2019-04-09","No","No","No","Internal"]
[null,null,null,null,2771,"22_20/10/2019 5:21:40 PM","2019-08-25","Defect","Ship Staff","Ship Staff Insp.","Slight leak from valve actuator of COV 509","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.11","Medium","","","Top actuator seal renewed.","2019-09-20","","Completed","2019-09-29","No","No","No","Internal"]
[null,null,null,null,2766,"22_2019-10-20 03:19:17.000","2019-08-26","Defect","Ship Staff","Ship Staff Insp.","Dressor coupling on Cargo line No. 2 iwo 4C leaking","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.1","Very High","","","Renewed","2019-09-10","","Completed","2019-08-31","No","No","No","Internal"]
[null,null,null,null,2767,"22_2019-10-20 04:11:51.000","2019-08-26","Defect","Ship Staff","Ship Staff Insp.","COW line valve on 2C leaking","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.33","Medium","","","Repaired","2019-09-18","","Completed","2019-04-09","No","No","No","Internal"]
[null,null,null,null,2770,"22_20/10/2019 5:20:30 PM","2019-08-29","Defect","Ship Staff","Ship Staff Insp.","Deck seal (semi dry type) kinetic pressure valve between U-seal and deck seal, flap broken","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.27","Medium","","","Flap repaired onboard and refitted","2019-01-09","","Completed","2019-08-31","No","No","No","Internal"]
[null,null,null,null,9960,"22_1/20/2020 2:05:36 PM","2019-08-29","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","No.1 DGPS Antenna securing arrangement needed renewal ","Navigation - GMDSS & Communication","General Appearance","External Factors","","","","","The person incharge and associated crew briefed about the importance of proper health of antennas. The monthly checks to be done more carefully and thoroughly ","2019-11-27","","Completed","2019-08-29","No","No","No","Internal"]
[null,null,null,null,9961,"22_1/20/2020 2:07:10 PM","2019-08-29","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Bridge Bell book not signed by the Officer of the watch. ","Navigation - Others","Navigation","Human Error","","","","","Training conducted for all the officers on the importance of making correct and complete entries in the ship`s log books. ","2019-11-27","","Completed","2019-08-29","No","No","No","Internal"]
[null,null,null,null,2623,"22_2019-10-12 06:19:17.000","2019-08-30","Breakdown","Ship Staff","Ship Staff Insp.","VECS System pressure reading in CCR not accurate.","Inert Gas","Cargo / Ballast Systems","Equipment Related","8.25","Very High","","","V to I convertor has been replaced, Calibration has been done by simulator. now Guage is in CCR showing the correct pressure. ","2019-12-30","DFAL190244","Completed","2019-10-28","No","No","No","Internal","to be completed on priority on receipt of spares"]
[null,null,null,null,2625,"22_2019-10-12 06:27:47.000","2019-08-30","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Paint faliure noted on many areas on deck","Miscellaneous","General Appearance","Equipment Related","11.4","Very High","","","duplicated in observation raised on 10-July-2019.","2020-01-30","","Completed","2020-10-01","No","No","No","Internal","date revised, more paints required for the job. RO to be forwarded for supply at Singapore Jan 20"]
[null,null,null,null,2626,"22_2019-10-12 06:30:05.999","2019-08-30","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","The Cargo and Marpol line has rust patches near midship area","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.4","Very High","","","De-rusting and painting near midship area for MARPOL line and cargo line completed","2020-05-05","","Completed","2020-04-05","No","No","No","Internal","work in progress; more paints supplied at last call Singapore ; revised completion date, kindly complete by then"]
[null,null,null,null,2627,"22_2019-10-12 06:33:49.999","2019-08-30","Defect","Ship Staff","Ship Staff Insp.","The anchor chain clearing rod is bent on both the gypsies","Deck - Mooring Machinery","Mooring","Equipment Related","9.2","Very High","","","DD Spec prepared in Refman. Deffered to Drydock","2021-07-31","","Completed","2020-04-05","Yes","No","No","Internal","the rod is bent, how ever it performs the task of clearing the cable of gypsy. planned renewal next docking. please forward the REFMAN export"]
[null,null,null,null,2640,"22_2019-10-12 06:12:29.999","2019-08-30","Breakdown","Ship Staff","Ship Staff Insp.","lifeboat stbd side steering gear system gear worn out condition","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.28","Very High","","","Recieved required spares and ractified.","2019-10-15","DFAL190237","Completed","2019-10-10","No","No","No","Internal"]
[null,null,null,null,7332,"22_Sat Oct 12 2019 06:19:17 GMT+0000 (Coordinated Universal Time)","2019-08-30","Breakdown","Ship Staff","Ship Staff Insp.","VECS System pressure reading in CCR not accurate.","Inert Gas","Cargo / Ballast Systems","Equipment Related","8.25","Very High","","","V to I convertor has been replaced, Calibration has been done by simulator. now Guage is in CCR showing the correct pressure. ","2019-12-30","DFAL190244","Completed","2019-10-28","No","No","No","Internal"]
[null,null,null,null,2768,"22_20/10/2019 5:16:55 PM","2019-08-30","Defect","Ship Staff","Ship Staff Insp.","Flow in IG Deck seal filling line very low","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.27","Medium","","","Completed","2019-01-09","","Completed","2019-07-09","No","No","No","Internal"]
[null,null,null,null,2769,"22_20/10/2019 5:18:52 PM","2019-08-30","Defect","Ship Staff","Ship Staff Insp.","AUS discharge to Slp (S) line developed leak during de-rusting","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.8","Medium","","","2 sections of lines repaired and refitted","2019-01-09","","Completed","2019-06-09","No","No","No","Internal"]
[null,null,null,null,2772,"22_20/10/2019 5:23:12 PM","2019-08-30","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Many lifebuoy lines found in very poor condition.","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.31","High","","","Renewed lines of lifebuoys.","2019-10-30","","Completed","2019-09-27","No","No","No","Internal"]
[null,null,null,null,8685,"22_Fri Dec 20 2019 23:54:26 GMT+0000 (Coordinated Universal Time)","2019-08-30","Defect","Ship Staff","Ship Staff Insp.","COP #2 leak from the seal","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","11.4","Very High","","","Leak was observed while discharging in initial stages (drops) later on No leak was observed at same RPM, same rectified","2019-10-30","","Completed","2019-10-26","No","No","No","Internal"]
[null,null,null,null,8686,"22_Fri Dec 20 2019 23:56:32 GMT+0000 (Coordinated Universal Time)","2019-08-30","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Lifeboat painter release mechanism found not working. The heliograph in poor condition.","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.31","High","","","Renewed after passing Singapore","2019-10-30","","Completed","2019-10-26","No","No","No","Internal"]
[null,null,null,null,8687,"22_Fri Dec 20 2019 23:57:52 GMT+0000 (Coordinated Universal Time)","2019-08-30","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Antenna supports found rusted and wasted.","Navigation - GMDSS & Communication","Navigation","Equipment Related","4.11","Medium","","","de-rusted and painted","2019-09-30","","Completed","2019-10-27","No","No","No","Internal"]
[null,null,null,null,8688,"22_Sat Dec 21 2019 00:01:00 GMT+0000 (Coordinated Universal Time)","2019-08-30","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","FBB GPS antenna has damage on top. Also the antenna is placed right under the dome, same can be shifted to a better location near the dome after construction with Mr. Kamlesh Solanki.","Navigation - GMDSS & Communication","Navigation","Equipment Related","4.11","Medium","","","Location of antenna found satisfactory for reception. Temporary repair is done on the antenna top.","2019-09-30","","Completed","2019-10-27","No","No","No","Internal"]
[null,null,null,null,2645,"22_17/10/2019 5:47:36 AM","2019-09-03","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","BA Compressor filling hose, leakage from sealing ring","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.43","High","","","Replaced with spare sealing ring & ordered new spares","2019-10-03","DFAL190108","Completed","2019-10-03","No","No","No","Internal"]
[null,null,null,null,9962,"22_1/20/2020 2:09:41 PM","2019-09-05","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","All though the Nav areas and T and P notices were Auto plotted on the ENC but same were not manually verified.","Navigation - Others","Navigation","Inappropriate Procedure","","","","","All warnings are manually verified against ADC and Nav warnings received by Mail by two officers indiviually. \n\nRecords for verification of T&P are mainatined in NP 133 C.\n\nAnd records for plotting of Navarea are mainatined in NAV Warning file. ","2019-08-06","","Completed","2019-06-12","No","No","No","Internal"]
[null,null,null,null,8682,"22_Fri Dec 20 2019 23:47:41 GMT+0000 (Coordinated Universal Time)","2019-09-07","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Deck steam (Inlet and return) line U-clamps to be derusted / painted and renewed where required.","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.7","High","","","Deck steam lines corroded U-Clamps renewed","2020-05-05","","Completed","2020-01-05","No","No","No","Internal","complete after the paints are received at Singapore 13 jan 20"]
[null,null,null,null,2775,"22_20/10/2019 5:29:38 PM","2019-09-10","Defect","Ship Staff","Ship Staff Insp.","Crude oilwashing line dressor coupling fwd of midship leaking","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.33","Medium","","","Renewed seal rings of dressor coupling","2019-09-10","","Completed","2019-09-10","No","No","No","Internal"]
[null,null,null,null,2622,"22_2019-10-12 06:08:20.000","2019-09-30","Defect","Ship Staff","Ship Staff Insp.","Mooring winch M5 leak from winch motor (inner motor)","Deck - Mooring Machinery","Mooring","Equipment Related","9.14","Medium","","","Renewed the hydraulic motor","2019-12-25","","Completed","2019-12-19","No","No","No","Internal","to be completed on priority before passing Singapore and follow up in separate mail"]
[null,null,null,null,8681,"22_Fri Dec 20 2019 23:44:57 GMT+0000 (Coordinated Universal Time)","2019-10-07","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Main deck coating breakdown from mid ship to poop deck and helicopter area","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.7","High","","","Port side main deck spot chipping / painting completed","2020-05-20","","Completed","2020-05-17","No","No","No","Internal","More sea stock paints supplied at Singapore 13 jan \nRevised completion date ; try to complete by then"]
[null,null,null,null,2628,"22_2019-10-12 06:38:31.000","2019-10-09","Defect","Ship Staff","Ship Staff Insp.","2P, 4P & 4S cargo tank hi-hi level alarm resistance tape faulty","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.24","Medium","","","2P, 4P & 4S resistance tape( sensor) has been renewed, High level alarms tried out, working satisfactorily.","2019-12-31","DFAL190264","Completed","2019-10-16","No","No","No","Internal","spares connected, kindly close out the job upon completion of repairs"]
[null,null,null,null,2776,"22_20/10/2019 5:31:51 PM","2019-10-13","Defect","Ship Staff","Ship Staff Insp.","IG dressor coupling leaking","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.22","Very High","","","Dressor coupling tightened and checked, no leak observed.","2019-10-13","","Completed","2019-10-13","No","No","No","Internal"]
[null,null,null,null,2778,"22_21/10/2019 5:48:58 PM","2019-10-15","Breakdown","Owner / Marine / Tech. Suptd.","Suptd. Insp.","stay wires for vsat antenna to renew","Navigation - GMDSS & Communication","Communication","External Factors","4.6","Medium","","","Renewed with new wire ropes","2020-01-15","","Completed","2019-10-31","No","No","No","Internal"]
[null,null,null,null,2629,"22_20/10/2019 5:37:49 PM","2019-10-16","Defect","Ship Staff","Ship Staff Insp.","Cable for BNWAS reset unit on Stbd. side bridge wing not secured to Bulwark","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.7","High","","","Effective Securing carried","2019-10-30","","Completed","2019-12-16","No","No","No","Internal"]
[null,null,null,null,2630,"22_20/10/2019 5:40:25 PM","2019-10-16","Defect","Ship Staff","Ship Staff Insp.","Stbd side wing light nut and bolt missing","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.7","High","","","Spot derusting carried out. New Bolt & Nut Fixed.","2019-10-31","","Completed","2019-10-27","No","No","No","Internal"]
[null,null,null,null,2631,"22_2019-10-22 04:06:56.999","2019-10-16","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Helipad area cosmetics to improve.","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.7","High","","","duplicated in observation raised on 10-July-2019.","2020-01-01","","Completed","2020-10-01","No","No","No","Internal","update in weekly reports"]
[null,null,null,null,2632,"22_2019-10-22 04:08:38.000","2019-10-16","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Bunker line near accommodation break to be painted","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.7","High","","","Bunker line near accommodation break painted","2020-01-01","","Completed","2019-12-15","No","No","No","Internal","reported completed , kindly confirm and close out"]
[null,null,null,null,2633,"22_2019-10-22 04:11:22.000","2019-10-16","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Two fire hose boxes on main deck to replace with fabricated boxes in ER.","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.38","High","","","Fire hose boxes  replaced with new ones.","2020-10-01","","Completed","2019-10-29","No","No","No","Internal"]
[null,null,null,null,2634,"22_2019-10-22 04:16:10.000","2019-10-16","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Stbd Life boat platform gratings to renew.","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.7","High","","","Hot work carried out. Old gratings Cropped. New gratings inserted & Fitted Using clamps","2020-01-02","","Completed","2020-01-21","No","No","No","Internal","gratings supplied in singapore; work in progress"]
[null,null,null,null,2635,"22_2019-10-22 04:17:22.000","2019-10-16","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Scupper drain forward of acetylene room to repair.","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.7","High","","","REPAIRED","2020-01-01","","Completed","2019-10-29","No","No","No","Internal","complete by 15th DEC and close out"]
[null,null,null,null,2636,"22_2019-10-22 04:18:51.999","2019-10-16","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","M5 mooring winch minor oil weep from flange to rectify.","Deck - Mooring Machinery","Mooring","Equipment Related","9.16","High","","","Control unit bolts re-tightened with Allen key bolts","2019-12-30","","Completed","2019-12-15","No","No","No","Internal","revised completion date 30 DEC. Close out on priority"]
[null,null,null,null,2637,"22_2019-10-22 04:19:42.999","2019-10-16","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Gantry crane to paint.","Deck - Machinery","General Appearance","Equipment Related","11.7","High","","","Painting of Gantry crane completed","2020-05-15","","Completed","2020-04-16","No","No","No","Internal","paints rcd at Singapore 13 jan , kindly complete before the target date"]
[null,null,null,null,2638,"22_2019-10-22 04:20:33.000","2019-10-16","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Ship side railings to clean and paint.","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.7","High","","","Ship side railings  cleaned and painted.","2020-06-30","","Completed","2020-12-06","No","No","No","Internal","kindly complete by target date; paints rcd at Singapore 13 Jan"]
[null,null,null,null,2639,"22_2019-10-22 04:24:07.000","2019-10-16","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","COW valve for 2centre not holding well, to overhaul or renew.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.34","High","","","Repaired. Renewed with a new one.","2019-11-12","","Completed","2019-11-12","No","No","No","Internal","arranged supply passing Singapore/ close out on priority"]
[null,null,null,null,7335,"22_Tue Oct 22 2019 04:08:38 GMT+0000 (Coordinated Universal Time)","2019-10-16","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Bunker line near accommodation break to be painted","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.7","High","","","Bunker line stenciling done by engine room staff in midship, port & starboard side.","2020-01-01","","Completed","2019-10-30","No","No","No","Internal"]
[null,null,null,null,7336,"22_Tue Oct 22 2019 04:11:22 GMT+0000 (Coordinated Universal Time)","2019-10-16","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Two fire hose boxes on main deck to replace with fabricated boxes in ER.","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.38","High","","","Fabrication of new Fire Hose boxes carried out. New Brackets welded after taking Concurrance from office","2020-10-01","","Completed","2019-10-29","No","No","No","Internal"]
[null,null,null,null,7337,"22_Tue Oct 22 2019 04:17:22 GMT+0000 (Coordinated Universal Time)","2019-10-16","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Scupper drain forward of acetylene room to repair.","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.7","High","","","Hot work carried out. Fabricated insert fitted","2020-01-01","","Completed","2019-10-29","No","No","No","Internal"]
[null,null,null,null,7338,"22_Tue Oct 22 2019 04:18:51 GMT+0000 (Coordinated Universal Time)","2019-10-16","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","M5 mooring winch minor oil weep from flange to rectify.","Deck - Mooring Machinery","Mooring","Equipment Related","9.16","High","","","Control unit bolts re-tightened with allen key bolts","2019-12-30","","Completed","2019-11-15","No","No","No","Internal"]
[null,null,null,null,7339,"22_Tue Oct 22 2019 04:24:07 GMT+0000 (Coordinated Universal Time)","2019-10-16","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","COW valve for 2centre not holding well, to overhaul or renew.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.34","High","","","Renewed with new Valve recieved at singapore. Renewal carried out","2019-11-12","","Completed","2019-11-11","No","No","No","Internal"]
[null,null,null,null,6081,"22_43760.1834143519","2019-10-16","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","COW valve for 2centre not holding well, to overhaul or renew.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.34","High","","","Renewed with new Valve recieved at singapore. Renewal carried out","2019-11-15","","Completed","2019-02-11","No","No","No","Internal"]
[null,null,null,null,2764,"22_2019-10-19 03:47:05.000","2019-10-16","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","starboard side gangway air leak ","Deck - Machinery","General Appearance","Equipment Related","11.7","High","","","Air hose coupling tightned, no leak.","2019-10-23","","Completed","2019-10-19","No","No","No","Internal"]
[null,null,null,null,2777,"22_20/10/2019 5:34:10 PM","2019-10-16","Defect","Ship Staff","Ship Staff Insp.","Stbd. side MOB marker support angle broken","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.31","High","","","Same fabricated and now in state of readiness.","2019-10-20","","Completed","2019-10-20","No","No","No","Internal"]
[null,null,null,null,2779,"22_21/10/2019 5:53:52 PM","2019-10-16","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","two accomodation door closers on stbd side to renew","Accommodation","General Appearance","Equipment Related","11.1","High","","","Old damaged Door closers renewed with new ones","2019-12-16","","Completed","2019-10-21","No","No","No","Internal"]
[null,null,null,null,2780,"22_21/10/2019 6:00:54 PM","2019-10-16","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","stbd gangway securing wires to renew","Deck - Machinery","Structural Condn. / WT integrity ","Equipment Related","","","","","New wire rope splicing carried out & refitted","2020-01-01","","Completed","2019-10-28","No","No","No","Internal"]
[null,null,null,null,2781,"22_2019-10-22 04:22:30.000","2019-10-16","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Cargo line #2 dresser coupling on top of #4 COT seal rings to renew.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.8","Medium","","","All three Cargo line dresser coupling seal rings on top of #4 COT renewed.","2019-10-23","","Completed","2019-10-21","No","No","No","Internal"]
[null,null,null,null,9454,"22_1/7/2020 1:37:32 AM","2019-10-25","Non Conformity","Owner / Marine / Tech. Suptd.","Ship Staff Insp.","Deck Stores Not Provided To Vesssel Due To Technical Errors In PAL ","Miscellaneous","Crew Management","Human Error","","","","","Vessel to send continuous reminders at short intervals so that office can revert with VFF in sufficient time and vessel can verify if there have been any technical glitches as reported above","2019-12-20","","Completed","2019-12-16","No","No","No","Internal"]
[null,null,null,null,9976,"22_1/20/2020 2:44:22 PM","2019-10-25","Non Conformity","Ship Staff","Ship Staff Insp.","Deck Stores Not Provided To Vesssel Due To Technical Errors In PAL ","Miscellaneous","Crew Management","Inappropriate Procedure","","","","","Vessel to send continuous reminders at short intervals so that office can revert with VFF in sufficient time and vessel can verify if there have been any technical glitches as reported above","2019-12-23","","Completed","2019-12-01","No","No","No","Internal"]
[null,null,null,null,9977,"22_1/20/2020 2:46:37 PM","2019-10-25","Non Conformity","Ship Staff","Ship Staff Insp.","VFF Sent To Vessel Very Late, Just Few Hours Prior Arrival At Singapore. \n\nMany important spares removed from Request List due to budget issues without verifying with Master ","Documentation","Cert. & Docu.","Human Error","","","","","Vessel to send continuous reminders at short intervals so that office can revert with VFF in sufficient time and vessel can verify if there have been any technical glitches as reported above","2019-12-23","","Completed","2019-12-01","No","No","No","Internal"]
[null,null,null,null,7330,"22_Mon Dec 16 2019 07:26:34 GMT+0000 (Coordinated Universal Time)","2019-10-28","Defect","Ship Staff","Ship Staff Insp.","Pumproom lights four gland packings  have worn out look , require replacement.","Elect. Mach. & Equip.","Cargo / Ballast Systems","Equipment Related","8.48","Medium","","","Pumproom lights gland packings replaced","2020-05-17","DFAL190214","Completed","2019-12-31","No","No","No","Internal","kindly complete on priority once the spares are received.\nspares delivered at Singapore- please close out on priority/ some machining required on the spares supplied. job to be completed soon. job reported to be closed out, please review and close out"]
[null,null,null,null,9956,"22_1/20/2020 1:39:03 PM","2019-11-07","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","One Pump room light cover found cracked. ","Cargo Mach.","Cargo / Ballast Systems","Inappropriate Procedure","","","","","The light cover for pumproom light was renewed with spare cover onboard.","2019-11-09","","Completed","2019-07-15","No","No","No","Internal"]
[null,null,null,null,9957,"22_1/20/2020 1:42:02 PM","2019-11-07","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Scrubber Tower: Open/close marking on all three W/T doors were not painted.","Hull & Tanks","Structural Condn. / WT integrity ","Human Error","","","","","All the markings were marked on doors for open/shut.","2019-11-09","","Completed","2019-12-07","No","No","No","Internal"]
[null,null,null,null,9958,"22_1/20/2020 1:44:11 PM","2019-11-07","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Scrubber Tower: A piece of pipe on all three W/T doors to tighten the dog leg clamps was not found.","Elect. Mach. & Equip.","Structural Condn. / WT integrity ","Human Error","","","","","During routine rounds after departure yard the shortcomings to be noted and ratified.","2019-11-09","","Completed","2019-07-17","No","No","No","Internal"]
[null,null,null,null,9959,"22_1/20/2020 2:02:00 PM","2019-11-07","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","On board complaint procedure was not found in officers smoke room.","Accommodation","Crew Management","Human Error","","","","","During sunday accommodation rounds, all required policies and procedures required posting to be checked and if found missing to be reposted. ","2019-11-09","","Completed","2019-07-12","No","No","No","Internal"]
[null,null,null,null,7340,"22_16/12/2019 7:18:39 AM","2019-11-11","Defect","Ship Staff","Ship Staff Insp.","IG scrubber pump disch. Elbow holed & gasket leaking.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Pump  isolated, elbow taken out for repair & , built up work carried out, gasker renewed and fitted in place. Pump tried out and found no leakages.","2019-12-05","","Completed","2019-11-12","No","No","No","Internal"]
[null,null,null,null,2662,"22_17/10/2019 6:53:43 AM","2019-11-15","Defect","Ship Staff","Ship Staff Insp.","No. 1 Hydrophore pump and DW pump to overhaul","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.1","Medium","","","No. 1 Hydrophore pump overhauled with new spares. pump tried out satisfactory","2019-12-31","","Completed","2019-12-24","No","No","No","Internal","raise RO for spares and complete the job on receipt of spares"]
[null,null,null,null,7329,"22_Mon Dec 16 2019 07:23:33 GMT+0000 (Coordinated Universal Time)","2019-11-23","Defect","Ship Staff","Ship Staff Insp.","FWG DISTILLATE PUMP CASING RINGS WORN OUT, MOTOR BEARING HOUSING WORN OUT, PUMP MOTOR NOT GETTING ALIGNED.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.1","Medium","","","TEMPORARY REPAIRS CARRIED OUT. PUMP OPERATING SATISFACTORILY. PO RECIEVED : DFAL 190200 AT SINGAPORE 22-DEC-2019. WE WILL INSTALL ASAP.","2019-12-31","","Completed","2019-12-22","No","No","No","Internal","close out and revert, already overdue"]
[null,null,null,null,9972,"22_1/20/2020 2:34:29 PM","2019-12-07","Non Conformity","Owner / Marine / Tech. Suptd.","Suptd. Insp.","C/E Mr. Sanjay Gaikwad- during bunkering and handing over at singapore anchorage \n\nNo minimum 6 hour consecutive rest period\n\nLess than 10 hour total rest in 24 hour period","Documentation","Crew Management","External Factors","","","","","next time onwards, we will plan well in advance during such port operations, so that the work and rest hours procedure could be followed. example, 2/E will relieve C/E during bunkers.","2019-07-31","","Completed","2019-08-12","No","No","No","Internal"]
[null,null,null,null,9968,"22_1/20/2020 2:27:22 PM","2019-12-22","Non Conformity","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Vessel was transisting Malacca Straits, Hardening Measures were taken, but one accomdation door was missed out which was reported during safety / security rounds to be closed. ","Accommodation","ISPS Related","Behaviour Based","","","","","ll doors should be manually checked. It should not be left to the responsibility of one person to do all. Members living on specific deck should also recheck for their own personnel safety and also ship's safety to avod such lapse in future.","2019-12-22","","Completed","2019-12-22","No","No","No","Internal"]
[null,null,null,null,10606,"22_2/27/2020 5:44:23 PM","2020-02-27","Observation","Owner / Marine / Tech. Suptd.","Cargo Audit","Date and time not written in the Pre arrival and commencement of cargo checklist Part B (24 hrs prior operation).","Documentation","Cargo / Ballast Systems","Human Error","8.8","Medium","","","Corrective:\n\nDate & Time Corrected/written on the Checklist \n\nPreventive: \n\nChecklist to be filled with due deligence for each & every entry & with accurate Date/timings. Same to be filed inside the Record file only after accurate checks being carried out for completion. \n\nDate closed: 27-Feb-2020\n\n","2020-02-29","","Completed","2020-02-27","No","No","No","Internal"]
[null,null,null,null,10607,"22_2/27/2020 5:47:31 PM","2020-02-27","Observation","Owner / Marine / Tech. Suptd.","Cargo Audit","Draining of lines - It is not specified which tank it is being drained into.","Documentation","Cargo / Ballast Systems","Human Error","6.6","Medium","","","Corrective:\n\nDraining of lines - specified with the Tank it is Drained.\n\nPreventive:\n\nPrior & after disconnection of manifolds, the Tank/s the manifolds are drained to be mentioned. Chief officer to ensure that the Entries carried out by OOW are checked for compliance.\n\nDate closed: 27-Feb-2020\n\n","2020-02-29","","Completed","2020-02-27","No","No","No","Internal"]
[null,null,null,null,10608,"22_2/27/2020 5:49:30 PM","2020-02-27","Observation","Owner / Marine / Tech. Suptd.","Cargo Audit","Pre arrival and commencement of cargo check list point # 1 not ticked.","Documentation","Cargo / Ballast Systems","Human Error","8.8","Medium","","","Corrective:\n\nPre arrival and commencement of cargo check list point # 1 ticked/corrected.\n\nPreventive: \n\nChecklist to be filled with due deligence for each & every entry. Same to be filed inside the Record file only after accurate checks being carried out for completion.\n\nDate closed: 27-Feb-2020 \n\n","2020-02-29","","Completed","2020-02-27","No","No","No","Internal"]
[null,null,null,null,10609,"22_2/27/2020 5:52:25 PM","2020-02-27","Observation","Owner / Marine / Tech. Suptd.","Mooring Audit","Mooring Winches not sighted marked with Max design BHC as per provided pictures.","Deck - Mooring Machinery","Mooring","Human Error","9.7","Medium","","","Corrective:\n\nAll Mooring winches marked with the Ship Design MBL.\n\nPreventive: \n\nProper marking to be done out including re-stencilling after any maintenance/painting jobs on the Mooring winches carried out. \n\nDate closed: 27-Feb-2020    \n\n","2020-02-29","","Completed","2020-02-27","No","No","No","Internal"]
[null,null,null,null,10610,"22_2/27/2020 5:57:15 PM","2020-02-27","Observation","Owner / Marine / Tech. Suptd.","Cargo Audit","Vessel carried out Ballasting operations at Yantai, China on 05 June 2020 and ballast water was discharged in Singapore port limits on 14 Jan 2020 without undergoing treatment or ballast exchange which is a violation of Ballast water convention.( AS PER ENTRY IN RECORD OF BALLAST WATER OPERATIONS)","Documentation","Cargo / Ballast Systems","Human Error","2.13","Low","","","Corrective:\n\nPlease be advised that vessel pumped out water from the afterpeak. Water inside the after peak was taken at Sea (Depth>1000 Mtrs; Distance from shore: >50nm).\n\nSame water was deballasted at Singapore. No water was ballasted inside APT from Yantai. ballasting at Singapore only because water was taken at sea & to reduce the Trim as per Bunker Surveyors request.\n\nPreventive:\n\nVessel to plan Water ballast exchange inside the South China Sea, if any planned Bunkering to take place at Singapore.\n\nDate closed: 27-Feb-2020\n\n","2020-02-29","","Completed","2020-02-27","No","No","No","Internal"]
[null,null,null,null,10611,"22_2/27/2020 9:47:11 PM","2020-02-27","Observation","Owner / Marine / Tech. Suptd.","Bunkering Audit","Repetitive checks were not carried out as per bunker safety checklist \n\n(It states every 2 hour, check list completed at 2300 but 1st signature of repetitive checks was carried out at 0200 hrs. Same mistake repeated again 0245 to 0500)\n\n","Documentation","MARPOL Related","Human Error","10.8","Medium","","","Corrective Action:\n\nDiscussed with Engineers with respect to maintaining the repetitive check intervals and to record the same as stated in the checklist \"within every 2Hrs'. \n\n\n\n","2020-02-29","","Completed","2020-02-27","No","No","No","Internal"]
[null,null,null,null,9445,"22_1/7/2020 2:32:44 AM","2020-03-01","Defect","Ship Staff","Ship Staff Insp.","4S COT VALVE (COV-914) UNABLE TO OPERATE REMOTELY FROM CCR. SAME TRIED OUT LOCALLY USING HYDRAULIC HAND PUMP- FREELY OPENING & CLOSING. SUSPECTED SOLENOID VALVE BLOCKAGE.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.11","Medium","","","FUNCTION OF SOLENOID VALVE HAVE BEEN CHECKED WORKING SATISFACTORY. VALVE TO OPENED/INSPECTED FOR MOVEMENT OF SPOOL PIECE, FOUND SPOOL PIECE STUCK. OVERHAULING/FREEING OF SPOOL PIECE CARRIED OUT DOUBLE PILOT CHECK VALVE TO INSPECTED. VESSEL TO ORDER FOR SUITABLE SPARES IN THE FUTURE","2020-03-03","","Completed","2020-11-01","No","No","No","Internal","Revert with complete troubleshooting and assistance required ."]
[null,null,null,null,9446,"22_1/7/2020 2:37:14 AM","2020-03-01","Defect","Ship Staff","Ship Staff Insp.","4S WBT VALVE (BWV-214) UNABLE TO OPERATE  REMOTELY FROM CCR . TRIED OUT LOCALLY USING HYDRAULIC HAND PUMP- FREELY OPENING & CLOSING. SUSPECTED SOLENOID VALVE BLOCKAGE.","Hull & Tanks","Cargo / Ballast Systems","Equipment Related","8.11","Medium","","","FUNCTION OF SOLENOID VALVE HAVE BEEN CHECKED WORKING SATISFACTORY. VALVE TO OPENED/INSPECTED FOR MOVEMENT OF SPOOL PIECE, FOUND SPOOL PIECE STUCK. OVERHAULING/FREEING OF SPOOL PIECE CARRIED OUT DOUBLE PILOT CHECK VALVE TO INSPECTED. VESSEL TO ORDER FOR SUITABLE SPARES IN THE FUTURE.","2020-03-03","","Completed","2020-11-01","No","No","No","Internal","carry out troubleshooting and revert.\nraise RO as required."]
[null,null,null,null,10804,"22_3/17/2020 11:22:45 AM","2020-03-13","Defect","Ship Staff","Ship Staff Insp.","Solenoid valve of 1 port WBT not working","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.11","Medium","","","Solenoid valve for 1 Port WBT replaced , now working satisfactory","2020-06-30","DFAL 200046","Completed","2020-06-15","No","No","No","Internal","spares arranged, close out on priority once the spares are rcd."]
[null,null,null,null,10805,"22_3/17/2020 11:29:13 AM","2020-03-13","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Mid ship hose handling crane platform bolts to renew","Deck - Machinery","General Appearance","Equipment Related","8.5","Very High","","","All midship crane platform bolts renewed","2020-02-05","","Completed","2020-06-05","No","No","No","Internal","staging and bolts supplied at Singapore-18 april,  kindly carry out the job after departure Singapore 24th april"]
[null,null,null,null,11423,"22_3/23/2020 8:31:09 AM","2020-03-20","Defect","Ship Staff","Ship Staff Insp.","AE F.O FLOW METER ( INLET & OUTLET ) NOT WORKING","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","AE FLOW METER DEFECTIVE PARTS REPLACED , FLOW METER PUT IN USE WORKING SATISFACTORY","2020-05-31","DFAL 200084","Completed","2020-06-17","No","No","No","Internal","spares processed,  will be connected  once ready at the earliest."]
[null,null,null,null,10481,"22_12/02/2020 8:03:35 AM","2020-04-02","Defect","Ship Staff","Ship Staff Insp.","When HFO 1(s) has been put in use , water content in purifier showing high and in settling tank drain water content was observed more than normal .","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Steam heating coil inlet and return line has been blanked. Leaking heating coil has been identified .At the earliest oppurtunity tank entry will be made to identify the exact location of the leak . Line to be repaired in DD.","2020-07-31","","Completed","2020-06-07","No","No","No","Internal","To be investigated , once the tank is empty and the defective coil to be blanked and Job to be included in REFMAN for repairs"]
[null,null,null,null,11424,"22_4/16/2020 2:29:52 AM","2020-04-15","Defect","Ship Staff","Ship Staff Insp.","MAIN ENGINE ACTUAL RPM PICKUP SENSOR SHOWING WRONG VALUE","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Technician attended , one card has been replaced , at present ME RPM pickup sensor showing accurate value","2020-05-15","","Completed","2020-04-18","No","No","No","Internal","service arranged at Singapore 18th April and close out; report in PAL under unplanned"]
[null,null,null,null,11695,"22_5/1/2020 4:30:15 AM","2020-04-20","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Air duct in steering gear room corroded","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","11.5","Medium","","","DD SPECS PREPARED IN REFMAN . JOB DEFFERED TO DRYDOCK","2021-09-30","","Completed","2020-05-19","Yes","No","No","Internal"]
[null,null,null,null,11696,"22_4/21/2020 3:53:35 AM","2020-04-20","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Outdoor unit condition is not very good, plan replacement","Miscellaneous","General Appearance","Equipment Related","11.3","Medium","","","Outdoor unit corroded section  cropped and renewed","2020-07-20","","Completed","2020-05-15","No","No","No","Internal","mention RO number  ; planned for supply  & replace around  mid july"]
[null,null,null,null,11697,"22_4/21/2020 3:57:22 AM","2020-04-20","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Hydroblaster maintenance to be done prior to the paint supply at Singapore and also check the condition of slury and grit blaster. All the machines to be put in use once the paints is received at Singapore","Deck - Machinery","General Appearance","Equipment Related","11.3","Medium","","","Hydroblaster and grit blaster tried out ,working in satisfactory condition Hydroblaster used for chipping of spare anchor","2020-05-20","","Completed","2020-05-14","No","No","No","Internal"]
[null,null,null,null,11698,"22_4/21/2020 4:03:59 AM","2020-04-20","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Pipe turning and renewal job in progress; target to complete the remaining job in next 2M","Deck - Pipe / Fittings","Mooring","Equipment Related","11.4","Very High","","","Hydraulic pipelines turning and renewal Completed","2020-06-20","","Completed","2020-05-25","No","No","No","Internal"]
[null,null,null,null,11699,"22_5/1/2020 4:18:32 AM","2020-04-20","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ME turning gear oil leak ","E/R - Main Engine","Eng. / Strg. Comp.","External Factors","10.29","Medium","","","Leak identified from the body where the screws were removed and tightened back in place with thread seal, presently no leakage.","2020-07-31","","Completed","2020-07-15","No","No","No","Internal"]
[null,null,null,null,11700,"22_5/1/2020 4:34:58 AM","2020-04-20","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Noise of air leak near ME emergency control station; to find source of leak and rectify","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Air leak has been identified , air leak arrested.","2020-07-15","","Completed","2020-08-07","No","No","No","Internal","kindly plan at load port, if there is any safe anchorage"]
[null,null,null,null,11701,"22_5/1/2020 4:38:05 AM","2020-04-20","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","FW Hydrofor pump Leaking; raise RO for mech seal type pump. In the meantime repair the existing pumps.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Existing pumps repaired. No leakage found. Also will be receivng mechanical type pumps. ","2020-08-15","DFAL200104","Completed","2020-11-08","No","No","No","Internal"]
[null,null,null,null,11702,"22_5/1/2020 4:41:59 AM","2020-04-20","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Valve bonett cut near LO transfer pump. Replace the valve bonnet or complete valve","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Broken valve repaired by welding and placed back , working satisfactory","2020-06-15","","Completed","2020-04-05","No","No","No","Internal"]
[null,null,null,null,11705,"22_5/1/2020 4:22:06 AM","2020-04-20","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Steering gear room top cleaning of stringers and equipment required","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","11.5","Medium","","","Area cleaned ","2020-04-30","","Completed","2020-04-29","No","No","No","Internal"]
[null,null,null,null,11706,"22_5/1/2020 4:25:18 AM","2020-04-20","Critical Equipment","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Water in emergency fire pump space to investigate and rectify","Critical Equip.","Eng. / Strg. Comp.","Equipment Related","10.31","Very High","","","Water leak observed from pump gland same has been nipped up . Emg. Fire pump area water cleaned","2020-04-30","","Completed","2020-04-20","No","No","No","Internal"]
[null,null,null,null,11707,"22_5/1/2020 4:39:54 AM","2020-04-20","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Overhauled spare ME exh valves, the oil ports and air ports not sealed well to prevent internal corrosion ","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Overhauled spare ME exh valves, the oil ports and air ports sealed properly with masking tape","2020-04-27","","Completed","2020-04-27","No","No","No","Internal"]
[null,null,null,null,11708,"22_4/21/2020 3:34:39 AM","2020-04-20","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Crew laundry and change room needs improvement in housekeeping","Accommodation","General Appearance","Inappropriate Procedure","11.13","Low","","","Crew laundry and changing rooms cleaned ","2020-04-30","","Completed","2020-04-27","No","No","No","Internal"]
[null,null,null,null,11709,"22_4/21/2020 3:47:44 AM","2020-04-20","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Fire line on deck all the U bolts wasted to be renewed","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.5","Medium","","","Fire line on deck all the wasted  U bolts replaced","2020-04-28","","Completed","2020-04-25","No","No","No","Internal"]
[null,null,null,null,11710,"22_4/21/2020 3:51:28 AM","2020-04-20","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Port side windlass Big gear top cover, one aft section part wasted, to renew","Deck - Mooring Machinery","General Appearance","Equipment Related","11.5","Medium","","","DD Spec prepared in Refman. Deffered to Drydock","2020-05-20","","Completed","2020-01-05","Yes","No","No","Internal"]
[null,null,null,null,11711,"22_4/21/2020 3:45:23 AM","2020-04-20","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","One foam monitor gratings thinned down around 2C COT. Replacement required","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.5","Medium","","","Grating near 2C COT for foam monitor cropped and renewed","2020-05-05","","Completed","2020-06-05","No","No","No","Internal"]
[null,null,null,null,11712,"22_4/21/2020 4:00:15 AM","2020-04-20","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Upper deck alleyway dim appearance. Paint floor with light green and bulkheads white","Accommodation","General Appearance","Inappropriate Procedure","11.13","Low","","","Uppde deck alleyway painting carried out","2020-05-20","","Completed","2020-05-05","No","No","No","Internal"]
[null,null,null,null,11713,"22_4/21/2020 3:41:02 AM","2020-04-20","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Officers smoke room ,wal need to be scrubbed to remove yellow stains","Accommodation","General Appearance","Inappropriate Procedure","11.13","Low","","","Officers smoke room wall scrubbed , yellow stains have faded after cleaning ,cleaned with detergent soap and scrubbed","2020-04-30","","Completed","2020-04-29","No","No","No","Internal"]
[null,null,null,null,11704,"22_5/1/2020 4:04:50 AM","2020-04-24","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","MAIN DECK STBD SIDE FWD OF MANIFOLD NEEDS TO BE CHIPPED AND PAINTED","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.3","Medium","","","MAINTAINANCE FOR MAIN DECK STBD SIDE IS IN PROGRESS","2020-07-24","","Completed","2020-06-28","No","No","No","Internal","complete and close out"]
[null,null,null,null,11703,"22_5/1/2020 4:02:47 AM","2020-04-25","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","SPARE ANCHOR FOUND TO BE RUSTED , SAME TO DERUST AND PAINT","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.3","Medium","","","SPARE ANCHOR HYDROBLASTING / PAINTING CARRIED OUT","2020-06-15","","Completed","2020-05-17","No","No","No","Internal","complete and close out"]
[null,null,null,null,10482,"22_12/02/2020 8:10:23 AM","2020-06-02","Defect","Ship Staff","Ship Staff Insp.","HFO Purifier No.2 water transducer showing erractic value. Water tarnsducer cleaned and interchanged with running Px and established faulty transducer.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Newly recieved spare fitted in place .Purifier tried out .Satisfactory","2020-04-20","DFAL200053","Completed","2020-01-05","No","No","No","Internal","spares processed for supply Feb 20; followup with purchase for supply"]
[null,null,null,null,12772,"22_6/18/2020 8:00:49 AM","2020-06-13","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","M/E Fuel Pump lay shaft to clean and grease.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","M/E Fuel Pump lay shaft cleaned and greased","2020-06-30","","Completed","2020-06-24","No","No","No","Internal","kindly complete as per target date and close out"]
[null,null,null,null,12773,"22_6/18/2020 8:05:13 AM","2020-06-13","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","E/R Port and Aft Bilge well’s to be de-mucked.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","E/R Port and Aft Bilge well’s demucked , cleaned and painted.","2020-08-10","","Completed","2020-10-08","No","No","No","Internal","kindly complete as per target date and close out"]
[null,null,null,null,12774,"22_6/18/2020 8:06:44 AM","2020-06-13","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ME aft main air cooler minor weeping marks from end cover without pipe connections","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","ME aft main air cooler end cover bolt tightened, weeping marks cleaned and painted. Presently no leakage.","2020-08-31","","Completed","2020-09-07","No","No","No","Internal","kindly complete as per target date and close out"]
[null,null,null,null,12775,"22_6/18/2020 8:09:47 AM","2020-06-13","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","M/E spare Air Dryer unit to be mounted near the drier station, covered nicely and tagged","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","M/E spare Air Dryer unit mounted near the drier station. ","2020-07-31","","Completed","2020-11-07","No","No","No","Internal","kindly complete as per target date and close out"]
[null,null,null,null,12776,"22_6/18/2020 8:16:29 AM","2020-06-13","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Steering Gear Room some more old metal trash to be cleared","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Steering Gear Room  old metal trash removed and shifted to garbage area","2020-08-31","","Completed","2020-06-20","No","No","No","Internal","kindly complete as per target date and close out"]
[null,null,null,null,12777,"22_6/17/2020 7:45:36 AM","2020-06-13","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Few winch covers partially corroded, to repair","Deck - Mooring Machinery","General Appearance","Equipment Related","11.1","High","","","Repairing of corroded winch covers carried out. ","2020-08-13","","Completed","2020-07-27","No","No","No","Internal","kindly complete as per target date and close out"]
[null,null,null,null,12778,"22_6/17/2020 7:47:37 AM","2020-06-13","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Hydroblaster machine to be derusted and painted","Deck - Machinery","General Appearance","Equipment Related","11.1","High","","","Hydroblaster machine derusted and painted.","2020-07-13","","Completed","2020-04-07","No","No","No","Internal","kindly complete as per target date and close out"]
[null,null,null,null,12779,"22_6/18/2020 8:19:12 AM","2020-06-13","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","M/E Flywheel Pit to be cleaned","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","M/E Flywheel Pit area cleaned","2020-07-31","","Completed","2020-06-29","No","No","No","Internal","kindly complete as per target date and close out"]
[null,null,null,null,12780,"22_6/18/2020 8:22:40 AM","2020-06-13","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","FWG performance low, to investigate","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","FWG condenser and evaporator cleaning carried out. Air and brine ejector non return flap cleaned.  Feed water line orifice cleaned. Ejector pump suction filter cleaned. Presently performance is satisfactory.","2020-07-31","","Completed","2020-07-17","No","No","No","Internal","kindly complete as per target date and close out"]
[null,null,null,null,12781,"22_6/18/2020 8:24:45 AM","2020-06-13","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ME forward Stay friction pads broken, to be renewed and tightened as per torque","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Broken friction pads of ME forward stay renewed and tightened","2020-08-31","","Completed","2020-10-07","No","No","No","Internal","kindly complete as per target date and close out"]
[null,null,null,null,12782,"22_6/18/2020 8:27:06 AM","2020-06-13","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Sox Scrubber pump outline on COPT deck has minor weeping mark from weld.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Weeping marks repaired by cold work. Presently no leakage.","2020-06-30","","Completed","2020-07-07","No","No","No","Internal"]
[null,null,null,null,12783,"22_6/18/2020 8:30:42 AM","2020-06-13","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Sox Scrubber Outlet Pressure Switch Coupling Leak Inside the Scrubber Tower. To be rectified.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Sox Scrubber Outlet leaking Pressure Switch Coupling rectified","2020-07-15","","Completed","2020-06-28","No","No","No","Internal","kindly complete as per target date and close out"]
[null,null,null,null,12784,"22_6/18/2020 8:35:43 AM","2020-06-13","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Funnel interconnection exhaust pipes to be painted.","Miscellaneous","General Appearance","Equipment Related","11.4","Very High","","","Funnel interconnection exhaust pipes painted.","2020-08-31","","Completed","2020-07-20","No","No","No","Internal","kindly complete as per target date at suitable anchorage and close out"]
[null,null,null,null,12785,"22_6/18/2020 2:10:36 AM","2020-06-13","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Port windlass anchor chain stopper not seated properly, jammed","Deck - Machinery","Mooring","Equipment Related","9.2","Very High","","","Port windlass anchor chain stopper will be eased up and then properly placed on to the anchor chain","2020-07-13","","Completed","2020-06-25","No","No","No","Internal"]
[null,null,null,null,12786,"22_6/18/2020 8:17:52 AM","2020-06-13","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Minor leaks on ME alfa lub pr accumulator washers","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Minor leaks on ME alfa lub pr accumulator washers rectified","2020-08-10","","Completed","2020-07-31","No","No","No","Internal"]
[null,null,null,null,12787,"22_6/17/2020 7:55:20 AM","2020-06-13","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Aft Mooring Winch Gratings to be derusted and painted.","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.4","Very High","","","Aft Mooring Winch Gratings derusting and painting completed","2020-07-13","","Completed","2020-08-17","No","No","No","Internal"]
[null,null,null,null,12788,"22_6/18/2020 8:40:44 AM","2020-06-13","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","China passage to be cleared of garbage. Useful small dia pipes to be shifted to ER pipe stand.","Miscellaneous","General Appearance","Equipment Related","11.3","Medium","","","China passage cleared of garbage. Useful small dia pipes shifted to ER pipe stand.","2020-06-30","","Completed","2020-06-29","No","No","No","Internal","kindly complete as per target date and close out"]
[null,null,null,null,12789,"22_6/18/2020 7:57:19 AM","2020-06-13","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","M/E Alfa Lube Oil pump #1 seal minor leak","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","M/E Alfa Lube Oil pump #1 replaced with new one and old one kept as standby after overhauling","2020-06-30","","Completed","2020-06-26","No","No","No","Internal","kindly complete as per target date and close out.\nspare pump to be OH and kept ready for use with proper tag"]
[null,null,null,null,12790,"22_6/18/2020 8:38:40 AM","2020-06-13","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Scrubber tower air inlet on stbd bottom, cleaning and touch-up required","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Scrubber tower air inlet on stbd bottom, cleaning and touch-up carried out","2020-01-07","","Completed","2020-07-20","No","No","No","Internal","kindly complete as per target date and close out"]
[null,null,null,null,12791,"22_6/18/2020 8:12:40 AM","2020-06-13","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","A/E 2 Exhaust Gas duct after TC lagging to renew.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","All 3 A/E  Exhaust Gas duct after TC lagging renewed .","2020-06-20","","Completed","2020-06-18","No","No","No","Internal"]
[null,null,null,null,12792,"22_6/18/2020 8:28:40 AM","2020-06-13","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Sox Scrubber WS valve #1 on overboard line is leaking from gland","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Sox Scrubber WS valve #1 on overboard line gland leakage rectified","2020-06-20","","Completed","2020-06-18","No","No","No","Internal"]
[null,null,null,null,12793,"22_6/18/2020 8:52:19 AM","2020-06-13","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Minor air leak near ME emer maneuvering stand to locate and rectify.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Minor air leak near ME emer maneuvering stand located and rectified , will be constatnly monitored from time to time","2020-06-20","","Completed","2020-06-18","No","No","No","Internal"]
[null,null,null,null,12794,"22_6/17/2020 7:52:24 AM","2020-06-13","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Bridge and radio room few placed of cable penetrations need to cover with class approved putty","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.4","Very High","","","cable penetrations covered with class approved putty","2020-06-28","","Completed","2020-06-17","No","No","No","Internal"]
[null,null,null,null,12795,"22_6/17/2020 7:58:28 AM","2020-06-13","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Upper deck alley way to be painted machine green to improve the brilliance in the area.","Accommodation","General Appearance","Equipment Related","11.13","Low","","","Upper deck alley way Cleaned and painted machine green .","2020-07-13","","Completed","2020-06-17","No","No","No","Internal"]
[null,null,null,null,12818,"22_6/27/2020 6:37:52 AM","2020-06-27","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","CCTV cameras are not installed at designated locations","Miscellaneous","ISPS Related","Equipment Related","7.12","High","","","CCTV cameras installed and commisioned.","2020-09-30","","Completed","2020-10-09","No","No","No","Internal","office arrangement; spares to be supplied soon  as per company standards for installation."]
[null,null,null,null,12819,"22_29/06/2020 10:21:40 AM","2020-06-28","Observation","Ship Staff","Ship Staff Insp.","ME alpha lube booster pump Spider coupling to order and renew for port side pump","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Port side Pump overhauled. Spider coupling is prepared onboard and kept standby for future use.","2020-08-31","","Completed","2020-07-10","No","No","No","Internal","spares to be confirmed once the quotes are received"]
[null,null,null,null,13478,"22_7/23/2020 9:50:58 AM","2020-07-23","Critical Equipment","Ship Staff","Ship Staff Insp.","MF/HF GMDSS Radio unable to transmit messages.","Navigation - GMDSS & Communication","Communication","Equipment Related","4.23","High","","","Spares received at Fujairah and Shore technician rectified the defect.","2020-08-15","","Completed","2020-08-25","No","No","No","Internal","service arranged at Fuj- 21 Aug"]
[null,null,null,null,13713,"22_30/08/2020 10:46:28 PM","2020-08-20","Observation","Ship Staff","Ship Staff Insp.","ME Emcy manovering area VIT control presure regulators leaking","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Spare reducers fixed.","2020-10-31","DFAL205065","Completed","2020-10-21","No","No","No","Internal","SPARES PROCESSED FOR SUPPLY; WILL BE READY SOON FOR CONNECTION"]
[null,null,null,null,13717,"22_30/08/2020 10:52:23 PM","2020-08-21","Observation","Ship Staff","Ship Staff Insp.","ME aft Air cooler casing bottom leaking","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.31","Very High","","","leak rectified by welding doubler plate","2020-08-31","","Completed","2020-08-25","No","No","No","Internal"]
[null,null,null,null,14489,"22_01/11/2020 9:28:36 PM","2020-08-25","Defect","Ship Staff","Ship Staff Insp.","Emergency stop valve leaking","Deck - Machinery","Cargo / Ballast Systems","Equipment Related","8.1","Very High","","","Newly received valve installed.","2020-10-24","","Completed","2020-10-23","No","No","No","Internal"]
[null,null,null,null,13954,"22_11/09/2020 7:53:00 PM","2020-08-31","Observation","Ship Staff","Ship Staff Insp.","Fire detector heads base found brittle.","LSA / FFA","Eng. / Strg. Comp.","Equipment Related","5.35","Medium","","","base renewed","2021-01-31","DFAL200164","Completed","2021-01-18","No","No","No","Internal","spares connected, \ncomplete the job as planned."]
[null,null,null,null,13714,"22_9/1/2020 12:34:48 PM","2020-08-31","Defect","Ship Staff","Ship Staff Insp.","Port Side Pilot ladder winch air motor performance is slow. Needs Overhauling.","Deck - Machinery","Safety / LSA / FFA","Equipment Related","5.47","Medium","","","Air motor overhauled. Pilot ladder support craddles greased. Air filter oil replenished. Winch motor found working satisfactorily.","2020-09-15","","Completed","2020-09-09","No","No","No","Internal","kindly revert with more details after checks and any spare requirement."]
[null,null,null,null,13715,"22_01/09/2020 11:25:34 PM","2020-09-01","Observation","Ship Staff","Ship Staff Insp.","Deck seal pipe lines few sections partially choked.","E/R - Pipes/ valves & fittings","Cargo / Ballast Systems","Equipment Related","8.27","Medium","","","Engine room side pipe sections renewed.","2020-12-28","","Completed","2020-12-24","No","No","No","Internal","complete as planned and close out before discharge port"]
[null,null,null,null,13716,"22_01/09/2020 11:30:59 PM","2020-09-01","Observation","Ship Staff","Ship Staff Insp.","Ejector pump no1 discharge pressure low.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Pump inspected found suction eye clogged with shells, all shells removed, pump tried out pressure 5.8bar.","2020-09-25","","Completed","2020-09-04","No","No","No","Internal","check as planned and revert after OH"]
[null,null,null,null,13964,"22_16/09/2020 12:22:06 PM","2020-09-07","Observation","Ship Staff","Ship Staff Insp.","Deck seal pump inlet valve leaking","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","defective valve replaced with spare valve","2020-09-16","","Completed","2020-09-11","No","No","No","Internal"]
[null,null,null,null,13965,"22_16/09/2020 12:25:49 PM","2020-09-08","Observation","Ship Staff","Ship Staff Insp.","Steam leaking from valve flange of Incinerator Waste oil tank #1","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","steam gasket replaced with metaflex.","2020-09-16","","Completed","2020-09-11","No","No","No","Internal"]
[null,null,null,null,13955,"22_9/13/2020 9:29:20 AM","2020-09-13","Observation","Ship Staff","Ship Staff Insp.","Foundation bolts of Stbd Lifeboat winch found deteriorated","LSA / FFA","Safety / LSA / FFA","Equipment Related","12.14","High","","","All foundation bolts renewed.","2021-10-01","","Completed","2020-09-22","No","No","No","Internal","Completion date is revised and Job to be completed ASAP."]
[null,null,null,null,13956,"22_9/13/2020 9:34:58 AM","2020-09-13","Defect","Ship Staff","Ship Staff Insp.","Air leaking from tell tale hole of Pressure reducer of SCBA set.","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.35","Medium","","","Received New Set and replaced.","2020-10-12","DFAL200198","Completed","2020-11-10","No","No","No","Internal"]
[null,null,null,null,13957,"22_9/13/2020 9:39:42 AM","2020-09-13","Observation","Ship Staff","Ship Staff Insp.","Fireman's outfit Lower pant torn at the bottom from inside and 01 coat torn near the waist area","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.35","Medium","","","New Sets received & replace.","2020-12-10","DFAL200199","Completed","2020-10-10","No","No","No","Internal","spares confirmed at Singapore for supply"]
[null,null,null,null,13958,"22_9/13/2020 9:46:54 AM","2020-09-13","Observation","Ship Staff","Ship Staff Insp.","Master call point switch on bridge is not close to steering stand","Miscellaneous","ISM Related","Equipment Related","4.1","High","","","Master call point switch relocated close to steering stand","2020-10-12","","Completed","2020-10-18","No","No","No","Internal","carry out as planned"]
[null,null,null,null,13959,"22_9/13/2020 9:57:36 AM","2020-09-13","Defect","Ship Staff","Ship Staff Insp.","Forward Draft Gauge showing Erratic Reading","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.12","Medium","","","To follow up with troubleshooting and raise requisition for spares as required. Forward draft guage compared visually at different draft found 20cm difference.","2020-10-12","","Completed","2020-12-27","No","No","No","Internal","awaiting follow up mail"]
[null,null,null,null,13960,"22_9/13/2020 9:59:38 AM","2020-09-13","Observation","Ship Staff","Ship Staff Insp.","Three PV Valves' vaccuum side wire mesh corroded","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.4","Medium","","","All three PV Valves Vaccuum side Wire mesh renewed. ","2020-12-10","","Completed","2020-09-17","No","No","No","Internal"]
[null,null,null,null,13961,"22_9/13/2020 10:02:21 AM","2020-09-13","Observation","Ship Staff","Ship Staff Insp.","Pump room exhaust vent wire mesh supporting frame corroded.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","5.18","High","","","Fabricated & Renewed Supporting frame and Wire mesh","2021-01-31","","Completed","2021-01-11","No","No","No","Internal","please plan in the ballast leg after Qingdao"]
[null,null,null,null,13962,"22_9/13/2020 10:06:13 AM","2020-09-13","Defect","Ship Staff","Ship Staff Insp.","One honey well impact pro gas detector pump Fault warning","Miscellaneous","Safety / LSA / FFA","Equipment Related","8.31","High","","","Replacement of the unit received at Port Qingdao. New gas detector working Satisfactorily","2020-09-30","","Completed","2020-09-25","No","No","No","Internal","arranged for supply at Qingdao"]
[null,null,null,null,13966,"22_9/13/2020 9:42:33 AM","2020-09-13","Defect","Ship Staff","Ship Staff Insp.","Limit switch at Stbd lifeboat manual hand cranking handle mounting not working","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","Limit switch replaced with the spare onboard. ","2020-09-16","","Completed","2020-09-13","No","No","No","Internal"]
[null,null,null,null,13963,"22_16/09/2020 12:31:24 PM","2020-09-14","Observation","Ship Staff","Ship Staff Insp.","Pin hole on EGE feed pump #1 suction line.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","new pipe line fabricated and installed","2020-09-17","","Completed","2020-09-16","No","No","No","Internal","close out as planned"]
[null,null,null,null,14134,"22_01/10/2020 1:27:06 PM","2020-09-27","Observation","Ship Staff","Ship Staff Insp.","Various power sockets in engine room damaged","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.37","Medium","","","power sockets need to be changed","2020-10-20","","Completed","2020-11-08","No","No","No","Internal","REVERT WITH RO ON PRIORITY FOR SUPPLY AT SINGAPORE"]
[null,null,null,null,14490,"22_16/10/2020 3:18:20 PM","2020-10-04","Observation","Ship Staff","Ship Staff Insp.","Drinking water hydraphore pump outlet valve inoperational.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","valcve replaced with new spare screwdown non return valve.","2020-10-19","","Completed","2020-10-14","No","No","No","Internal"]
[null,null,null,null,14483,"22_10/15/2020 7:52:16 AM","2020-10-10","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Self-closing device is corroded and broken on E-deck port side entrance","Accommodation","General Appearance","Equipment Related","5.1","Very High","","","Self closing door renewed","2020-11-11","","Completed","2020-10-11","No","No","No","Internal","complete and close out as planned."]
[null,null,null,null,14484,"22_10/15/2020 8:27:59 AM","2020-10-10","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Port side life boat fenders at stow position was not adjusted in actual position. Condition of fender is deteriorated and damaged partially","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.28","Very High","","","Life boat fenders to be renewed, requisition raised awaiting supply.  ITEM RECEIVED, RENEWAL OF FENDERS IN PROGRESS.","2021-02-28","DAFL200255","Completed","2021-02-28","No","No","No","Internal","spares rcd and closed out"]
[null,null,null,null,14485,"22_10/15/2020 8:38:02 AM","2020-10-10","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Fwd. winch drums and windlass  was sighted with thick rust","Deck - Machinery","General Appearance","Equipment Related","11.1","High","","","Derusting and painting completed","2020-12-12","","Completed","2020-10-12","No","No","No","Internal","complete and close out as planned"]
[null,null,null,null,14486,"22_10/15/2020 8:51:43 AM","2020-10-10","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Hydraulic inlet and outlet valve wheel was missing at Valve control box near 2C and 1C tank lid","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","6.4","High","","","valve wheel replaced.","2020-12-12","DFAL200292","Completed","2020-01-12","No","No","No","Internal","Raise RO if no spares onboard.\ncomplete and close out as planned. spares to be processed for supply"]
[null,null,null,null,14491,"22_10/15/2020 8:14:51 AM","2020-10-10","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Scuppers at the brake of accommodation port and stbd side was found leaking. Rubber part of the scupper was  deteriorated","Miscellaneous","MARPOL Related","Equipment Related","6.2","High","","","Scupper Replaced ","2020-11-11","","Completed","2020-10-15","No","No","No","Internal"]
[null,null,null,null,14492,"22_10/15/2020 7:57:10 AM","2020-10-10","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Em. Generator exhaust vent was sighted with thick rust.","Miscellaneous","General Appearance","Equipment Related","5.1","Very High","","","De rusting and painting of Em. Generator exh vent completed.","2020-10-11","","Completed","2020-10-16","No","No","No","Internal"]
[null,null,null,null,14493,"22_10/15/2020 9:04:21 AM","2020-10-10","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Pump room natural vent (stbd) mesh support was found with heavy rust and partially damaged","Miscellaneous","General Appearance","Equipment Related","5.18","High","","","Derusting and painting carried out.","2020-11-11","","Completed","2020-10-30","No","No","No","Internal"]
[null,null,null,null,14494,"22_10/15/2020 8:35:18 AM","2020-10-10","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","No. 8 valve control box on deck was sighted with heavy rust.","Deck - Machinery,Miscellaneous","General Appearance","Equipment Related","11.1","High","","","Derusting and painting carried out.","2020-11-11","","Completed","2020-10-30","No","No","No","Internal"]
[null,null,null,null,14500,"22_15/10/2020 5:57:33 PM","2020-10-10","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Crew mess, smoking room door self-closing mechanism was not working","Accommodation","Safety / LSA / FFA","Equipment Related","11.6","Medium","","","Self closing mechanism adjusted. ","2020-11-12","","Completed","2020-10-15","No","No","No","Internal"]
[null,null,null,null,15932,"22_12/16/2020 8:43:15 AM","2020-10-11","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Diesel oil dresser Coupling Gasket found leaking.","Deck - Pipe / Fittings","MARPOL Related","Equipment Related","6.5","Medium","","","Diesel oil Dresser coupling gasket renewed","2020-12-31","","Completed","2020-12-15","No","No","No","Internal"]
[null,null,null,null,14941,"22_19/11/2020 11:32:04 AM","2020-10-11","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Boiler blow down pipe bottom section heavily corroded, cracked,","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.31","Very High","","","New pipe to fabricated, installed","2020-11-27","","Completed","2020-11-21","No","No","No","Internal","complete as planned"]
[null,null,null,null,14488,"22_15/10/2020 6:06:42 PM","2020-10-11","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Rating pantry door self-closing door mechanism is not working and no rubber packing.","Accommodation","MLC Related","Equipment Related","5.1","Very High","","","self closing door mechanism need renewed and door silencers renewed.","2020-11-12","","Completed","2020-11-18","No","No","No","Internal","raise RO and  include in DDRL as well"]
[null,null,null,null,14495,"22_15/10/2020 5:36:57 PM","2020-10-11","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","P/room entrance W/T door from stbd side  was found with a damaged gasket/packing.","Accommodation,Miscellaneous","Structural Condn. / WT integrity ","Equipment Related","10.44","Medium","","","Damaged packing renewed and checked for W/T integrity.","2020-11-11","","Completed","2020-10-27","No","No","No","Internal"]
[null,null,null,null,14497,"22_01/11/2020 9:37:33 PM","2020-10-16","Defect","Ship Staff","Ship Staff Insp.","#2 ME FO circulating pump discharge valve not holding, pump rotating in opposit e direction during stopped condition.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Valve replaced with spare valve.","2020-10-25","","Completed","2020-10-23","No","No","No","Internal"]
[null,null,null,null,14498,"22_01/11/2020 9:30:42 PM","2020-10-17","Defect","Ship Staff","Ship Staff Insp.","#3 AE fuel inlet valve not holding","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Valve replaced with spare","2020-10-30","","Completed","2020-10-24","No","No","No","Internal"]
[null,null,null,null,14499,"22_01/11/2020 9:35:01 PM","2020-10-18","Defect","Ship Staff","Ship Staff Insp.","Soot tank drain pipe holed.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.31","Very High","","","New pipe fabricated and installed","2020-10-25","","Completed","2020-10-20","No","No","No","Internal"]
[null,null,null,null,14487,"22_01/11/2020 9:32:54 PM","2020-10-28","Defect","Ship Staff","Ship Staff Insp.","Discharge pipe of Scrubber cooling sea water pump pin holed.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.31","Very High","","","Pipe section removed, fabrication of new section in progress.","2020-11-02","","Completed","2020-11-01","No","No","No","Internal","noted work complete; to be closed in the next report"]
[null,null,null,null,14501,"22_15/10/2020 6:12:09 PM","2020-11-10","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Exhaust of Galley hot plate was found with thick oil and fat","Accommodation","General Appearance","Behaviour Based","11.13","Low","","","Exhaust of galley hot plate cleaned. ","2020-10-11","","Completed","2020-10-15","No","No","No","Internal"]
[null,null,null,null,14943,"22_19/11/2020 11:26:54 AM","2020-11-14","Observation","Ship Staff","Ship Staff Insp.","Scrubber low level alarm float connecting flange holed.","Inert Gas","Eng. / Strg. Comp.","Equipment Related","10.31","Very High","","","New flange fabricated","2020-11-21","","Completed","2020-11-18","No","No","No","Internal"]
[null,null,null,null,14940,"22_19/11/2020 11:29:43 AM","2020-11-15","Observation","Ship Staff","Ship Staff Insp.","Aux Engine Fresh water cooler #1 sea water inlet pipe pin hole.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.31","Very High","","","Pipe fabricated","2020-11-21","","Completed","2020-11-28","No","No","No","Internal","complete as planned and close out"]
[null,null,null,null,14942,"22_19/11/2020 11:39:33 AM","2020-11-18","Observation","Ship Staff","Ship Staff Insp.","Boiler blow down valve SDNR not holding","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.31","Very High","","","Valve replaced","2020-12-05","","Completed","2020-12-02","No","No","No","Internal","kindly confirm if the correct rating of valve available for replacement"]
[null,null,null,null,15434,"22_30/11/2020 7:04:34 AM","2020-11-20","Observation","Ship Staff","Ship Staff Insp.","ME LO cooler sea water inlet pipe distance piece after the valve holed ","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.31","Very High","","","Distance piece renewed with fabricated spare.","2020-11-29","","Completed","2020-11-24","No","No","No","Internal"]
[null,null,null,null,15435,"22_30/11/2020 7:07:17 AM","2020-11-25","Observation","Ship Staff","Ship Staff Insp.","Aux No 2 HFO inlet valve not closing","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Valve repalced with spare","2020-11-30","","Completed","2020-11-29","No","No","No","Internal"]
[null,null,null,null,14135,"22_01/10/2020 1:24:15 PM","2020-11-30","Observation","Ship Staff","Ship Staff Insp.","HFO Settling tank gauge not working","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","GAUGE RENEWED. SATISFACTORY","2021-02-16","DFAL200216","Completed","2021-02-08","No","No","No","Internal","spares confirmed for supply, awaiting readiness"]
[null,null,null,null,14136,"22_01/10/2020 2:00:02 PM","2020-11-30","Observation","Ship Staff","Ship Staff Insp.","DO Tank capacity gauge faulty","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","GAUGE RENEWED.","2021-01-31","DFAL20219","Completed","2021-02-08","No","No","No","Internal","spares confirmed for supply, awaiting readiness"]
[null,null,null,null,15930,"22_17/12/2020 9:12:04 AM","2020-12-03","Observation","Ship Staff","Ship Staff Insp.","Steam leak from STBD bunker tank inlet valve bonnet","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Valve bonnet gasket replaced.","2020-12-11","","Completed","2020-12-08","No","No","No","Internal"]
[null,null,null,null,14496,"22_16/10/2020 3:20:26 PM","2020-12-10","Observation","Ship Staff","Ship Staff Insp.","M6 mooring winch stbd hydraulic motor inlet pipe facing area cracked.","Deck - Mooring Machinery","Mooring","Equipment Related","9.14","Medium","","","Housing interchanged from spare motor.","2020-10-20","","Completed","2020-10-19","No","No","No","Internal"]
[null,null,null,null,15931,"22_12/17/2020 5:41:43 AM","2020-12-12","Observation","Ship Staff","Ship Staff Insp.","Cosmetic Maintenance on Funnel to be carried out.","Miscellaneous","General Appearance","External Factors","11.8","Low","","","Chipping and painting work to be carried out after obtaining working aloft permission from office.","2020-12-31","","Completed","2020-12-14","No","No","No","Internal"]
[null,null,null,null,16520,"22_29/12/2020 6:18:26 PM","2020-12-25","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Control air quality for EGCS  to improve","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Auto drain to install in ECGS tower.Ordered Festo filters.                                                                               spares received and Auto drain filter  Installed in ECGS Scrubber Tower.  Put in Use and found working satisfactory.","2021-03-31","DFAL210026","Completed","2021-04-26","No","No","No","Internal","spares quotes awaited"]
[null,null,null,null,17425,"22_04/01/2021 4:47:30 PM","2021-01-02","Defect","Ship Staff","Ship Staff Insp.","Pressure transmitter giving erratic signal, effecting air compressor loading and unloading operation","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Pressure transmitter received and renewed. comntrol air compressor tried out. found in good working order.","2021-02-28","210005","Completed","2021-02-04","No","No","No","Internal","spare pr transmitter arranged for supply. to be connected at Singapore in the ballast leg"]
[null,null,null,null,17426,"22_04/01/2021 5:07:51 PM","2021-01-04","Observation","Ship Staff","Ship Staff Insp.","AE LO purifier 3way valve diaphram leaking, ","E/R - Purifier","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","spare received and renewed diaphram. purifier started and found in good working order.","2021-02-08","DFAL210012","Completed","2021-02-04","No","No","No","Internal","noted Ro raised for the spare; same will be arranged once the quotes are received."]
[null,null,null,null,18995,"22_3/4/2021 15:23:38","2021-01-04","Defect","Ship Staff","Ship Staff Insp.","Aft ETA pickup rope container's lid & release arrangement appear seized.","Deck - Machinery","Emgcy. Systems","Equipment Related","9.28","Medium","","","Lid/hinge/relase handles to be freed up. ALREADY FREED UP. ","2021-05-30","","Completed","2021-04-16","No","No","No","Internal","complete as planned and close out"]
[null,null,null,null,19004,"22_3/4/2021 13:55:53","2021-01-04","Defect","Ship Staff","Ship Staff Insp.","Pumproom flooding damper control operation from pumproom top found seized. ","Deck - Machinery","Cargo / Ballast Systems","Equipment Related","5.19","Medium","","","Overhaul/ operate on regular basis. OVERHAULED AND LUBRICATED PROPERLY, TESTED, FOUND OPERATIONAL. ","2021-04-15","","Completed","2021-05-04","No","No","No","Internal"]
[null,null,null,null,19005,"22_3/4/2021 13:59:22","2021-01-04","Breakdown,Defect","Ship Staff","Ship Staff Insp.","Navigation light housing & acrylic glass fitting broken from base due to weather exposure.","Deck - Machinery,Navigation - Others","Navigation","Equipment Related,External Factors","4.8","Medium","","","repaired","2021-05-30","","Completed","2021-05-09","No","No","No","Internal"]
[null,null,null,null,17652,"22_27/01/2021 9:34:46 AM","2021-01-20","Observation","Ship Staff","Ship Staff Insp.","Safety valve to install on control air bottle. Auto drain to fix on the drain connection of control and service air bottle","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Safety valve installed","2021-02-15","DFAL210047","Completed","2021-02-16","No","No","No","Internal","will be connected this call Singapore. complete and close out as planned"]
[null,null,null,null,17653,"22_27/01/2021 9:37:01 AM","2021-01-24","Observation","Ship Staff","Ship Staff Insp.","Fresh water genrator salinometer erratic at times","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","CONDENSER LEAKING TUBE PLUGGED. NOW SALINOMETER IS WORKING IN SATISFACTORY CONDITION","2021-03-13","DFAL210033","Completed","2021-03-08","No","No","No","Internal","spares to be confirmed soon for supply"]
[null,null,null,null,17654,"22_31/01/2021 6:36:17 PM","2021-01-25","Defect","Ship Staff","Ship Staff Insp.","Forward Fog Horne not operational","Navigation - Others","Navigation","Equipment Related","","","","","Air supply and electric circuit to be checked.Air supply and elecronic circuit checked and serviced.","2021-01-26","","Completed","2021-01-26","No","No","No","Internal"]
[null,null,null,null,17782,"22_2/8/2021 1:13:55 PM","2021-02-02","Defect,Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","The hydraulic boxes for cargo valves on deck – one side of the hinge had corroded and can no more serve as a locking arrangement – (see photo) lids to be taken to E/R w/shop and repaired asap.","Deck - Machinery","Cargo / Ballast Systems","Equipment Related","11.4","Very High","","","E/R WORKSHOP FOR FABRICATION OF HINGES, WORK IN PROGRESS. WORK DONE, SAME HAS BEEN RE-INSTALLED. PAINTING WORK DONE AFTER INSTALLATION.  ","2021-05-03","","Completed","2021-02-18","No","No","No","Internal","complete as planned"]
[null,null,null,null,17783,"22_09/02/2021 1:26:53 PM","2021-02-02","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Few hyd boxes on deck the sealing lip damage covered with temporary repairs","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","10.42","Medium","","","Two box cover temporary  repaired with material onboard. all defective box covers to be repaired in DD. REFMAN to be updated accordingly.  REFMAN UPDATED WITH DEFECTIVE BOX COVERS. MATERIAL TO BE PROCURED BEFORE DD. REQ TO BE RAISED","2021-08-30","","Completed","2021-04-30","Yes","No","No","Internal","work in progress, to be completed as planned"]
[null,null,null,null,17784,"22_09/02/2021 1:29:06 PM","2021-02-02","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Mast riser drain line valve handle damaged and line in poor condition","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.19","High","","","handle and line to be renewed. JOB IN PROGRESS.","2021-03-03","","Completed","2021-02-28","No","No","No","Internal","complete and close out"]
[null,null,null,null,16519,"22_29/12/2020 6:22:47 PM","2021-02-02","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Deck seal filling pipe in pump room side clogged.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.27","Medium","","","damaged pipe fabricated. Now water flow is normal to the deck seal. Water level also satisfactory","2021-02-28","","Completed","2021-02-27","No","No","No","Internal","complete as planned and close out"]
[null,null,null,null,17799,"22_2/8/2021 1:06:45 PM","2021-02-02","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Scuppers on monkey island were found choked with debris ","Accommodation","General Appearance","Behaviour Based,Inappropriate Procedure","10.42","Medium","","","CLEANED, TESTED WITH WATER FOUND ALL SCUPPERS ARE CLEAR AND WORKING SATISFACTORY","2021-02-15","","Completed","2021-10-02","No","No","No","Internal"]
[null,null,null,null,17800,"22_2/8/2021 1:09:39 PM","2021-02-02","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Numerous anti-piracy hardening measurers around accommodation hinges are frozen and cannot be used effectively.","Accommodation","ISPS Related","Behaviour Based,Human Error,Inappropriate Procedure","7.12","High","","","FREEING AND CHIPPING/ PAINTING OF ALL ANTI-PIRACY HARDENING MEASURES AROUND ACCOMMODATION DONE","2021-03-04","","Completed","2021-11-02","No","No","No","Internal"]
[null,null,null,null,17801,"22_2/8/2021 1:19:09 PM","2021-02-02","Defect,Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","The main deck safe access to bow - cat walk grating was in poor condition and cud result in a personal accident","Deck - Machinery,Deck - Pipe / Fittings","ISM Related","Human Error,Inappropriate Procedure","11.1","High","","","GRATING RENEWED ","2021-02-15","","Completed","2021-11-02","No","No","No","Internal"]
[null,null,null,null,17802,"22_2/8/2021 1:21:29 PM","2021-02-02","Defect,Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Safety chains with safety hook arrangement around boat deck were found heavily corroded and hooks were also jammed","Deck - Pipe / Fittings,LSA / FFA","ISM Related","Behaviour Based,Human Error","8.64","Medium","","","CHIPPING / PAINTING AND FREEING OF BOTH SIDE BOAT DECK CHAINS DONE","2021-02-15","","Completed","2021-10-02","No","No","No","Internal"]
[null,null,null,null,17803,"22_2/8/2021 11:53:22 AM","2021-02-02","Non Conformity,Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","G’way equipment greasing was completed – but Oil meant for splash lubrication of gear was not renewed – no date of last change was also available.","Deck - Machinery","ISM Related","Behaviour Based,Equipment Related,Inappropriate Procedure,Knowledge Based","5.47","Medium","","","OVERHAULING OF OIL & AIR FILTERS OF BOTH GANGWAY DONE, OIL RENEWED IN ALL OIL FILTERS AND MOTOR GEAR BOX FOR SPLASH LUBRICATION, BUFFING AND PAINTING OF FILTER BOXES ALSO CARRIED OUT, ALL FOUND WORKING SATISFACTORY.","2021-03-03","","Completed","2021-02-13","No","No","No","Internal"]
[null,null,null,null,17804,"22_2/8/2021 11:58:51 AM","2021-02-02","Defect,Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","The water level gauge glass of the Deck Seal was opaque – reportedly pipelines were choked","Cargo Mach.,Deck - Machinery,Deck - Pipe / Fittings,Inert Gas","Cargo / Ballast Systems","Equipment Related","8.27","Medium","","","GAUGE GLASS REMOVED AND CLEANED AND REPLACED, FOUND IN GOOD WORKING CONDITION, FIND JOB IN WEEKLY WORK DONE REPORT.","2021-02-15","","Completed","2021-02-13","No","No","No","Internal"]
[null,null,null,null,17805,"22_2/8/2021 1:16:37 PM","2021-02-02","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","The mid ships stores was in poor state of housekeeping. Reducer presentation flanges were not protected – This is a rainy day job – Bosun to be tasked to bring it back to presentable condition and a fresh inventory taken","Miscellaneous","General Appearance","Behaviour Based,Human Error,Inappropriate Procedure","11.12","Low","","","MIDSHIP STORE ARRANGED, HEAVY ITEMS LASHED PROPERLY, REDUCERS BUFFED AND PAINTED, PLACED ON WOODEN SURFACE, FIND JOB DONE DETAILS IN WEEKLY WORK DONE REPORT. OBS COULD NOT BE CLOSED IN LPSQ MODULE IN PAL SINCE JOB FLOW ASSIGNED TO FLEET MANAGER","2021-02-15","","Completed","2021-02-13","No","No","No","Internal"]
[null,null,null,null,17787,"22_09/02/2021 1:24:50 PM","2021-02-03","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Old used drums are placed at Steering gear room and Forepeak store","Miscellaneous","Eng. / Strg. Comp.","Inappropriate Procedure","10.42","Medium","","","Old used drums from steering gear room and FPK store, stowed in scrubber tower 1st deck, and will be used for anti-piracy purpose.","2021-06-30","","Completed","2021-06-30","No","No","No","Internal","complete as planned"]
[null,null,null,null,19006,"22_15/04/2021 4:57:50 AM","2021-02-04","Observation","Ship Staff","Ship Staff Insp.","EMERGENCY GENERATOR HYDRAULIC STARTER IS NOT WORKING PROPERLY","Critical Equip.","Emgcy. Systems","Equipment Related","10.32","Very High","","","ACCUMMULATOR , REALY VALVE RENEWED.AND STARTER  OVERHAULED","2021-02-08","DFAL210061","Completed","2021-04-14","No","No","No","Internal"]
[null,null,null,null,17791,"22_09/02/2021 1:37:31 PM","2021-02-08","Observation","Ship Staff","Ship Staff Insp.","No 2 EGB feed pump pressure is very less","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Pump overhauled pressure is satisfactory","2021-03-06","210009","Completed","2021-02-20","No","No","No","Internal"]
[null,null,null,null,17798,"22_09/02/2021 1:34:49 PM","2021-02-08","Observation","Ship Staff","Ship Staff Insp.","No 1 EGB feed pump pressure is very less","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Pump  overhauled. pressure improved","2021-03-30","210009","Completed","2021-04-02","No","No","No","Internal","spares to be processed on priority."]
[null,null,null,null,17792,"22_10/02/2021 1:17:09 PM","2021-02-09","Critical Equipment","Ship Staff","Ship Staff Insp.","OWS BILGE HOLDING TANK TO BILGE HOLDING TANK CHANGE OVER COCK IS SLUGGISH","Critical Equip.,E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","6.14","High","","","COCK  EASED UP","2021-02-17","","Completed","2021-02-16","No","No","No","Internal","complete as planned and close out"]
[null,null,null,null,17806,"22_15/02/2021 12:32:05 PM","2021-02-09","Critical Equipment","Ship Staff","Ship Staff Insp.","EMERGENCY FIRE PUMP WAS FOUND NOT TAKING SUCTION DURING BALLAST CONDITION","Critical Equip.","Eng. / Strg. Comp.","Equipment Related","5.41","Very High","","","PRIMING PUMP LEVER OVERHAULED. PUMP IS TAKING SUCTION NOW","2021-02-11","","Completed","2021-02-10","No","No","No","Internal"]
[null,null,null,null,17794,"22_10/02/2021 1:19:01 PM","2021-02-10","Observation","Ship Staff","Ship Staff Insp.","MSB ROOM AIRCON SEA WATER INLET PIPE HAS LEAKAGES AT THREE PLACES","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","PIPE  RENEWED.","2021-02-21","","Completed","2021-02-16","No","No","No","Internal","job in progress to be completed as planned."]
[null,null,null,null,17807,"22_14/02/2021 8:15:30 AM","2021-02-11","Defect","Ship Staff","Ship Staff Insp.","EGCS SEA CHEST LEAKING","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","LEAKAGE RECTIFIED BY WELDING","2021-02-12","","Completed","2021-02-12","No","No","No","Internal"]
[null,null,null,null,17795,"22_14/02/2021 8:12:17 AM","2021-02-13","Observation","Ship Staff","Ship Staff Insp.","FWG EJECTOR PUMP NO 2 alignment to check","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","PUMP OVERHAULED AND FITTED BACK . MOTOR PROPERLY ALIGNED","2021-03-30","","Completed","2021-03-23","No","No","No","Internal","check as per planned and revert in separate mail with ROB od spares; plan OH of pump and motor as required"]
[null,null,null,null,17796,"22_14/02/2021 8:13:50 AM","2021-02-14","Observation","Ship Staff","Ship Staff Insp.","BOILER FEED PUMP NO 1 IS VIBRATING","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","ALIGNMENT DONE AND  FOUNDATION RETIGHTNED.","2021-03-30","","Completed","2021-03-07","No","No","No","Internal","check as per planned and follow up in separate mail"]
[null,null,null,null,17797,"22_15/02/2021 10:19:26 AM","2021-02-15","Defect","Ship Staff","Ship Staff Insp.","A/C CONDENSER DISCHARGE PIPE STUB PIPE HAS PIN HOLE.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","PIPE REPAIRED","2021-02-28","","Completed","2021-02-27","No","No","No","Internal","plan and replace at the load port if possible"]
[null,null,null,null,19008,"22_15/04/2021 4:54:39 AM","2021-02-16","Defect","Ship Staff","Ship Staff Insp.","STBD LIFEBOAT STEERING MECHANISM  HAS A CRACK","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.28","Very High","","","STEERING GEAR MECHANISM RENEWED. NOW WORKING IN GOOD CONDITION","2021-03-01","DFAL210062","Completed","2021-04-14","No","No","No","Internal"]
[null,null,null,null,18132,"22_02/03/2021 7:20:23 PM","2021-02-16","Breakdown,Critical Equipment,Non Conformity","Ship Staff","Ship Staff Insp.","some wire strand of L/B  falls wire broken. Wire only holding onto few strands.  Need to change the wire as soon as possible as more than 10% wire found damaged. ","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.29","High","","","RO to be raised. vessel has one set of wire as spare. Another two set raised for DD renewal. Presently working on to cut the damaged portion and to fix back onboard. RENEWAL OF THE PORT SIDE LIFE BOAT WIRE DONE WITH ONBOARD SPARE. ","2021-05-15","DFAL210074","Completed","2021-08-04","No","No","No","Internal"]
[null,null,null,null,19007,"22_15/04/2021 5:00:42 AM","2021-02-17","Critical Equipment","Ship Staff","Ship Staff Insp.","STBD LIFEBOAT BATTERY IS WEAK. NOT CHARGING PROPERLY","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.28","Very High","","","STBD LIFEBOAT BOTH BATTERY RENEWED","2021-04-05","DFAL210059","Completed","2021-04-14","No","No","No","Internal"]
[null,null,null,null,18139,"22_02/03/2021 7:44:50 PM","2021-02-19","Observation","Ship Staff","Ship Staff Insp.","All 3 Aux engine turbocharger insulation is defective","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","insulation  repaired. New insulation material to be ordered.","2021-03-05","","Completed","2021-03-04","No","No","No","Internal"]
[null,null,null,null,18134,"22_02/03/2021 7:46:35 PM","2021-02-20","Observation","Ship Staff","Ship Staff Insp.","Galley food disposer performance is less","Miscellaneous","MARPOL Related","Equipment Related","10.32","Very High","","","DISPOSER INSPECTED AND BLADES CLEANED.WORKING SATISFACTORILY.","2021-03-16","","Completed","2021-03-03","No","No","No","Internal","awaiting further info"]
[null,null,null,null,18136,"22_02/03/2021 7:39:06 PM","2021-02-25","Defect","Ship Staff","Ship Staff Insp.","Control air compressor Pressure sensor is erratic and oil separator are defective","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Pressure sensor and oil separator  renewed","2021-04-09","DFAL210065","Completed","2021-03-13","No","No","No","Internal","spares to be processed as per RO and to be connected at Singapore in ballast leg"]
[null,null,null,null,18138,"22_02/03/2021 7:23:38 PM","2021-02-27","Defect","Ship Staff","Ship Staff Insp.","Hydraulic main line coming to M7 winch corodded , found hydraulic oil leaking from damaged line, Fabrication job need to carry out  before arrival load port, section of pipe need to renew.","Deck - Mooring Machinery","Mooring","Equipment Related","9.16","High","","","Pipe  renewed.","2021-03-22","","Completed","2021-03-04","No","No","No","Internal","complete as planned"]
[null,null,null,null,18228,"22_09/03/2021 5:56:30 PM","2021-03-07","Defect","Ship Staff","Ship Staff Insp.","ABNORMAL SOUND NOTED FROM MAIN AIR COMPRESSOR NO 2 ","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","COMPRESSOR OVERHAULED ","2021-03-08","","Completed","2021-03-07","No","No","No","Internal"]
[null,null,null,null,18226,"22_15/03/2021 5:06:40 PM","2021-03-13","Defect","Ship Staff","Ship Staff Insp.","EMERGENCY FIRE PUMP SCUPPER DRAIN PIPE IS CHOCKED","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","BLOCKAGE CLEARED","2021-03-16","","Completed","2021-03-17","No","No","No","Internal","complete as planned and close out"]
[null,null,null,null,18227,"22_15/03/2021 5:09:26 PM","2021-03-14","Defect","Ship Staff","Ship Staff Insp.","STP DISCHARGE PUMP MECH SEAL LEAKING","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","PUMP OVERHAULED","2021-03-18","","Completed","2021-03-26","No","No","No","Internal","complete as planned and close out"]
[null,null,null,null,18404,"22_26/03/2021 3:22:15 PM","2021-03-22","Defect","Ship Staff","Ship Staff Insp.","ME TURBOCHARGER GRIT WASHING AIRLINE VALVES ARE LEAKING","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","VALVES RENEWED","2021-04-10","","Completed","2021-03-28","No","No","No","Internal"]
[null,null,null,null,18402,"22_26/03/2021 3:19:25 PM","2021-03-25","Defect","Ship Staff","Ship Staff Insp.","EGE CLEANING WATER DRAIN LINE WASTED AND PIPE DAMAGED. EXHAUST GAS SLIGHLY LEAKING","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","NEW PIPE FABRICATED AND FITTED","2021-05-17","","Completed","2021-05-30","No","No","No","Internal","kindly renew as planned and coat the new pipe with some scrubber overboard corrocoat paint"]
[null,null,null,null,19009,"22_3/4/2021 15:40:23","2021-04-01","Observation","Ship Staff","Ship Staff Insp.","Anti skid paints at some sections of walkway has been removed due to spot derusting/repainting. ","Deck - Pipe / Fittings,Miscellaneous","General Appearance","Knowledge Based","11.3","Medium","","","To apply anti skid paint on affected sections. ANTISKID PAINT APPLIED ON THE CHIPPED AREA FROM BREAK OF ACC UPTO BOTH SIDE MANIFOLD AREA. WILL CONTINUE TO PUT IN THE WALKWAY ONCE REQUIRED CHIPPING PAINTING IS CARRIED OUT. ","2021-07-30","","Completed","2021-04-15","No","No","No","Internal"]
[null,null,null,null,19010,"22_4/24/2021 6:26:19 AM","2021-04-01","Breakdown","Ship Staff","Ship Staff Insp.","STBD SIDE PUMP ROOM MECHANICAL SUPPLY FAN STAY WIRE BROKEN.","Deck - Machinery","Cargo / Ballast Systems","External Factors","5.18","High","","","BROKEN WIRE REPLACED WITH NEW ONE","2021-04-16","","Completed","2021-04-15","No","No","No","Internal"]
[null,null,null,null,19015,"22_05/04/2021 7:10:46 PM","2021-04-04","Observation","Ship Staff","Ship Staff Insp.","SEWAGE TREATMENT PLANT ELEMENTS BROKEN","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","ELEMENTS REPALCED WITH NEW SPARE","2021-04-06","","Completed","2021-04-06","No","No","No","Internal"]
[null,null,null,null,19011,"22_15/04/2021 4:45:55 AM","2021-04-07","Defect","Ship Staff","Ship Staff Insp.","GALLEY AIRCON BLOWER CASING COMPLETELY CORRODED AND DAMAGED.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","NEW CASING  FABRICATED.","2021-05-08","","Completed","2021-04-18","No","No","No","Internal"]
[null,null,null,null,19012,"22_14/04/2021 1:33:43 PM","2021-04-13","Defect","Ship Staff","Ship Staff Insp.","BOILER NO 1 F O CONTROLLER MAGNETIC COIL BURNT","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","CONTROLLER TO BE RENEWED. ","2021-04-17","DFAL210142","Completed","2021-05-19","No","No","No","Internal"]
[null,null,null,null,19013,"22_23/04/2021 9:28:40 AM","2021-04-20","Defect","Ship Staff","Ship Staff Insp.","IG BLOWER NO 1 MOTOR TRIPPED ON OVERLOAD AND IR IS SHOWING ZERO","Cargo Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","MOTOR OVERHAULED, CLEANED AND REVARNISHED. IMPROVED IR AND MOTOR BOXED BACK. MOTOR IS SATISFACTORY","2021-04-22","","Completed","2021-04-21","No","No","No","Internal"]
[null,null,null,null,19000,"22_30/04/2021 9:33:00 AM","2021-04-23","Defect","Ship Staff","Ship Staff Insp.","FEW CABIN'S MATTRESS IS DEFECTIVE","Accommodation","Crew Management","Equipment Related","8.55","Low","","","MATTRESS TO BE RENEWED. REQ RAISED. RECEIVED AT SINGAPORE ON 09-05-2021 AND REPLACED. ","2021-05-30","RO DFAL210151","Completed","2021-09-05","No","No","No","Internal","mattress to be supplied at Singapore."]
[null,null,null,null,19014,"22_28/04/2021 10:45:42 AM","2021-04-25","Observation","Ship Staff","Ship Staff Insp.","BILGE PUMP PRESSURE WAS VERY LESS","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","BILGE PUMP OVERHAULED AND PROBLEM RECTIFIED","2021-05-01","","Completed","2021-04-26","No","No","No","Internal"]
[null,null,null,null,19002,"22_28/04/2021 10:47:29 AM","2021-04-28","Defect","Ship Staff","Ship Staff Insp.","NO 2 BOILER WATER CIRCULATING PUMP IS VIBRATING","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","PUMP AND MOTOR OVERHAULED.","2021-05-16","","Completed","2021-05-01","No","No","No","Internal","complete as planned and revert with the findings"]
[null,null,null,null,19003,"22_28/04/2021 10:49:44 AM","2021-04-28","Defect","Ship Staff","Ship Staff Insp.","EGB OUTLET VALVE AND NO 2 BOILER WATER DRUM VALVE TO BOILER WATER CIRCULATING PUMP FOUND SEIZED AND HARD TO OPERATE","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","VALVES OVERHAULED","2021-06-01","","Completed","2021-05-01","No","No","No","Internal","plan and close out while awaiting cargo discharge in China or during singapore bunkering operations."]
[null,null,null,null,19451,"22_14/05/2021 9:32:35 AM","2021-05-04","Defect","Ship Staff","Suptd. Insp.","ME LO COOLER SEA WATER OUTLET STUB PIECE IS CORRODED","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","NEW STUB PIECES ARE FITTED IN PLACE FOR INLET AND OUTLET SECTION. ","2021-06-01","","Completed","2021-05-19","No","No","No","Internal","stub pipes ready for replacement. awaiting suitable time for completion of job"]
[null,null,null,null,19452,"22_14/05/2021 9:39:21 AM","2021-05-06","Observation","Ship Staff","Ship Staff Insp.","ICO LUBE SO OIL PERCENTAGE WAS NOTED SLIGHTLY HIGHER","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","FAULT RECTIFIED AFTER COMMUNICATION WITH MAKER.","2021-05-15","","Completed","2021-05-16","No","No","No","Internal","troubleshooting in progress with makers consultation"]
[null,null,null,null,19454,"22_14/05/2021 9:30:15 AM","2021-05-08","Observation","Ship Staff","Ship Staff Insp.","ER SLUDGE DISCHARGE LINE TO SLOP TANK IS CORRODED","Deck - Pipe / Fittings","MARPOL Related","Equipment Related","11.4","Very High","","","CORRODED SECTION RENEWED","2021-07-31","","Completed","2021-07-20","No","No","No","Internal","complete as planned and close out"]
[null,null,null,null,19458,"22_14/05/2021 9:41:04 AM","2021-05-10","Observation","Ship Staff","Ship Staff Insp.","SLIGHT WATER LEAKAGE NOTED FROM MAIN ENGINE NO 7 UNIT LINER COOLING WATER CONNECTION","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","COOLING WATER CONNECTION O RINGS  RENEWED.","2021-05-20","","Completed","2021-05-18","No","No","No","Internal","job planned for 17 may  ; weather permitting before crew change in India"]
[null,null,null,null,19456,"22_5/13/2021 3:06:25 PM","2021-05-13","Breakdown,Defect","Ship Staff","Ship Staff Insp.","DURING BWE FOUND 4P BALLAST TANK MAIN VALVE BEV 204 LEAKING, VALVE OPENING CLOSING FROM CCR AND LOCAL BUT STILL LEAKING. MAY BE SEAT RING DAMAGED.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","2.9","Medium","","","4 P WBT MAIN VALVE OPERATED AND TESTED FOR BALLASTING AND DEBALLASTING OPERATION, WORKING SATISFACTORY. DURING SHUT POSITION VALVE WAS HOLDING WITH ADJACENT TANK PRESSURE HEAD 2.5 BARS.","2021-05-31","","Completed","2021-05-20","No","No","No","Internal","awaiting further details; check ROB of seat rings and revert,"]
[null,null,null,null,19457,"22_15/05/2021 7:33:15 AM","2021-05-13","Observation","Ship Staff","Ship Staff Insp.","FBB ANTENNA FOUNDATION BASE IS CORRODED","Navigation - GMDSS & Communication","Communication","Equipment Related","4.2","Medium","","","Foundation base and support bracket for wire, spot de-rusted and painted. Foundation base thickness found satisfactory.","2021-06-30","","Completed","2021-12-06","No","No","No","Internal","complete as planned and close out"]
[null,null,null,null,19620,"22_1/6/2021 01:32:00","2021-05-26","Observation","Ship Staff","Ship Staff Insp.","Stbd Gangway slewing requires use of chain block. Hoisting speed for both gangways are much slower than usual & this results in delays. Motors seem underpowered & same need to be investigated.","Deck - Machinery","Safety / LSA / FFA","Equipment Related","5.47","Medium","","","Motor inspection carried out but no difference noted. All sheaves old grease removed and re-lubricated. Few sheaves and gangway channel spot derusting, painting and lubrication carried out. Gangway slewing slowly without use of chain block.","2021-01-09","","Completed","2021-04-06","No","No","No","Internal","revert in separate mail; let me know when were the air motors renewed. is there enough drive air pressure. are the pulleys free to rotate."]
[null,null,null,null,19621,"22_1/6/2021 01:46:34","2021-05-30","Observation","Ship Staff","Ship Staff Insp.","Bridge front lights & midship post lights are improperly focussed on deck. There are large areas on deck not illuminated at night.","Elect. Mach. & Equip.","General Appearance","Equipment Related","11.9","Low","","","Lights' brackts de-rusted, freed and lubricated. 3 Bulbs found not working and replaced ETO. Deck lights focussed properly on deck.","2021-01-07","","Completed","2021-06-23","No","No","No","Internal","complete and close out as planned."]
[null,null,null,null,19622,"22_1/6/2021 02:00:36","2021-05-31","Other","Ship Staff","Ship Staff Insp.","Treadmill at Gymnasium not usable as movement is jerky. Pilot at Rastanura expressed grievance that condition has not been rectified since his last visit 1 year ago.","Miscellaneous","MLC Related","Equipment Related","","","","","Treadmill investigated by ETO. Belt tightened & lubricated with silicon grease. ","2021-09-01","","Completed","2021-06-18","No","No","No","Internal","raise RO for new thread mill / No RO yet in the system"]
[null,null,null,null,20333,"22_7/24/2021 11:32:36 AM","2021-06-07","Defect","Ship Staff","Ship Staff Insp.","One UTI, Sr/No. R11880, was broken (frame and storage tube detached) and also showing 'No Msg' in display.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.12","Medium","","","UTI was sent ashore for service and repair. Broken parts and tape replaced. Now UTI working satisfactory. ","2021-07-31","DFAL215045 & DFAL210226","Completed","2021-07-12","No","No","No","Internal"]
[null,null,null,null,19938,"22_20/6/2021 15:35:12","2021-06-19","Defect","Ship Staff","Ship Staff Insp.","Frequest loud hammeriing/knocking on FW distribution line on bridge deck. The shock & vibration from repeated vibrations are likely to cause damage & leaks in pipeline. ","Deck - Pipe / Fittings,E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Hammering traced at faucet hot water line. HW line blanked as there is no stop cock in the supply lines to faucet. Same will be fitted upon receipt of stores. ","2021-09-19","","Completed","2021-06-23","No","No","No","Internal"]
[null,null,null,null,19939,"22_02/07/2021 3:46:00 PM","2021-06-26","Defect","Ship Staff","Ship Staff Insp.","DRINKING WATER HYDROPHORE PUMP SUCTION DISTANCE PIECE FOUND CRACK, NEEDS REPLACEMENT.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","NEW DISTANCE PIECE FABRICATED AND PUT IN PLACE.","2021-06-28","","Completed","2021-06-29","No","No","No","Internal"]
[null,null,null,null,19936,"22_7/1/2021 6:42:48 AM","2021-06-29","Other","Ship Staff","Ship Staff Insp.","During cargo operation, it was observed 3C cargo tank stripping valve SRV-923 not operating from CCR. We tried operating from local solenoid control, valve is operating however indicator shows shut position only.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.11","Medium","","","Local solenoid indicator and solenoid connection checked. Indicator panel replaced. Now SRV923 is operational from CCR.","2021-09-30","","Completed","2021-04-07","No","No","No","Internal","to be included for docking jobs, if unable to complete by then."]
[null,null,null,null,20151,"22_21/07/2021 7:02:46 PM","2021-07-01","Other","Ship Staff","Ship Staff Insp.","STORE ROOM IN STEERING GEAR COMPARTMENT DIRTY AND NOT ARRANGED","Miscellaneous","Eng. / Strg. Comp.","Behaviour Based","","","","","STORE ROOM CLEANED AND ARRANGED","2021-07-09","","Completed","2021-07-07","No","No","No","Internal"]
[null,null,null,null,20152,"22_21/07/2021 7:04:56 PM","2021-07-05","Other","Ship Staff","Ship Staff Insp.","ACCOMODATION A/C CONDENSER SEA WATER SIDE END COVER LEAKING","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","END COVER GASKET RENEWED.","2021-07-10","","Completed","2021-07-08","No","No","No","Internal"]
[null,null,null,null,20334,"22_8/3/2021 8:24:59 AM","2021-08-01","Defect","Ship Staff","Ship Staff Insp.","Ballast pipe line flange between strainer and ballast pump no.1, have pinhole leakage.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.11","Medium","","","Temporary repair carried out. During docking permanent repair will be carried out.","2021-09-30","","Completed","2021-08-01","No","No","No","Internal"]

{"sheet":"Calc","index":2,"n_rows":28,"n_cols":12,"rows_kept":28,"cut":false,"hidden":true,"merged":[]}
["Def_type","Def_cause","Equipments","VIQrefno","Observer_code"]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,"Dim itemSele As Long"]
[null,null,null,null,null,null,null,null,null,null,null,"   dim startRow as integer"]
[null,null,null,null,null,null,null,null,null,null,null,"   startRow=1"]
[null,null,null,null,null,null,null,null,null,null,null,"        For itemSele = 0 To ListBox1.ListCount - 1"]
[null,null,null,null,null,null,null,null,null,null,null,"        If ListBox1.Selected(itemSele) = True Then"]
[null,null,null,null,null,null,null,null,null,null,null,"        Worksheets(\"WorksheetName\").Range(\"A\" & startRow).Value = ListBox1.List(itemSele)"]
[null,null,null,null,null,null,null,null,null,null,null,"        startRow = startRow + 1"]
[null,null,null,null,null,null,null,null,null,null,null,"        End If"]
[null,null,null,null,null,null,null,null,null,null,null,"        Next"]
[null,null,null,null,null,null,null,null,null,null,null,"Dim LastRowA As String"]
[null,null,null,null,null,null,null,null,null,null,null,"        Dim itemSele As Long"]
[null,null,null,null,null,null,null,null,null,null,null,"       Dim startRow as integer"]
[null,null,null,null,null,null,null,null,null,null,null,"        LastRowA = ActiveSheet.Cells(Rows.count, \"A\").End(xlUp).row"]
[null,null,null,null,null,null,null,null,null,null,null,"        startQue = 0"]
[null,null,null,null,null,null,null,null,null,null,null,"        For itemSele = 0 To ListBox1.ListCount - 1"]
[null,null,null,null,null,null,null,null,null,null,null,"        For startRow = 1 To LastRowA"]
[null,null,null,null,null,null,null,null,null,null,null,"        If Worksheets(\"WorksheetName\").Range(\"A\" & startRow).Value = ListBox1.List(itemSele) Then"]
[null,null,null,null,null,null,null,null,null,null,null,"        ListBox1.Selected(itemSele) = True"]
[null,null,null,null,null,null,null,null,null,null,null,"        Exit For"]
[null,null,null,null,null,null,null,null,null,null,null,"        End If"]
[null,null,null,null,null,null,null,null,null,null,null,"        Next j"]
[null,null,null,null,null,null,null,null,null,null,null,"        Next"]
[null,null,null,null,null,null,null,null,null,null,null,"        End If"]

{"sheet":"Areaofobs","index":3,"n_rows":17,"n_cols":2,"rows_kept":17,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Cargo / Ballast Systems",11]
["Cert. & Docu.",2]
["Communication",6]
["Crew Management",3]
["Emgcy. Systems",13]
["Eng. / Strg. Comp.",14]
["General Appearance",15]
["Ice Opns.",17]
["ISM Related",7]
["ISPS Related",10]
["MARPOL Related",9]
["MLC Related",4]
["Mooring",12]
["Navigation",5]
["Safety / LSA / FFA",8]
["Structural Condn. / WT integrity ",16]

{"sheet":"Vessel_type","index":4,"n_rows":1,"n_cols":2,"rows_kept":1,"cut":false,"hidden":true,"merged":[]}
["Vessel_type","ID"]

{"sheet":"Deficiency_type","index":5,"n_rows":8,"n_cols":3,"rows_kept":8,"cut":false,"hidden":true,"merged":[]}
["TITLE","Type of deficiency_description","ID"]
["Breakdown",null,6]
["Critical Equipment",null,4]
["Defect",null,1]
["Guarantee Claim",null,8]
["Non Conformity",null,2]
["Observation",null,3]
["Other",null,7]

{"sheet":"VIQrefno","index":6,"n_rows":427,"n_cols":3,"rows_kept":427,"cut":false,"hidden":true,"merged":[]}
["VIQ_ref_no","Risk Value of observation","ID"]
["1.1","Low",8243]
["1.10","Low",8252]
["1.11","Low",8253]
["1.12","Low",8254]
["1.13","Low",8255]
["1.14","Low",8256]
["1.15","Low",8257]
["1.16","Low",8259]
["1.17","Low",8260]
["1.18","Low",8261]
["1.19","Low",8262]
["1.2","Low",8244]
["1.20","Low",8263]
["1.21","Low",8265]
["1.22","Low",8266]
["1.23","Low",8267]
["1.24","Low",8268]
["1.25","Low",8269]
["1.26","Low",8270]
["1.3","Low",8245]
["1.4","Low",8246]
["1.5","Low",8247]
["1.6","Low",8248]
["1.7","Low",8249]
["1.8","Low",8250]
["1.9","Low",8251]
["1.99","High",11258]
["10.1","Medium",8461]
["10.10","High",8470]
["10.11","Medium",8471]
["10.12","Very High",8472]
["10.13","Very High",8473]
["10.14","Medium",8474]
["10.15","Low",8475]
["10.16","Very High",8476]
["10.17","Very High",8477]
["10.18","High",8478]
["10.19","Very High",8479]
["10.2","Low",8462]
["10.20","High",8480]
["10.21","Medium",8481]
["10.22","Low",8482]
["10.23","Medium",8483]
["10.24","Low",8484]
["10.25","Very High",8485]
["10.26","High",8486]
["10.27","Medium",8487]
["10.28","Low",8488]
["10.29","Medium",8489]
["10.3","Medium",8463]
["10.30","High",8490]
["10.31","Very High",8491]
["10.32","Very High",8492]
["10.33","High",8493]
["10.34","High",8494]
["10.35","Very High",8495]
["10.36","Very High",8496]
["10.37","Medium",8497]
["10.38","Medium",8498]
["10.39","High",8499]
["10.4","High",8464]
["10.40","Medium",8500]
["10.41","Medium",8501]
["10.42","Medium",8502]
["10.43","Medium",8503]
["10.44","Medium",8504]
["10.45","Very High",8505]
["10.46","High",8506]
["10.47","Medium",8507]
["10.48","High",8508]
["10.49","Medium",8509]
["10.5","Low",8465]
["10.50","High",8510]
["10.51","Low",8511]
["10.52","Medium",8512]
["10.53","Medium",8513]
["10.54","High",8514]
["10.55","Low",8515]
["10.6","Very High",8466]
["10.7","Medium",8467]
["10.8","Medium",8468]
["10.9","Medium",8469]
["10.99","High",8516]
["11.1","High",8420]
["11.10","Medium",8429]
["11.11","Very High",8430]
["11.12","Low",8431]
["11.13","Low",8432]
["11.14","Medium",8433]
["11.15","Low",8434]
["11.16","Low",8435]
["11.17","Low",8436]
["11.2","Medium",8421]
["11.3","Medium",8422]
["11.4","Very High",8423]
["11.5","Medium",8424]
["11.6","Medium",8425]
["11.7","High",8426]
["11.8","Low",8427]
["11.9","Low",8428]
["11.99","High",8437]
["12.1","High",8438]
["12.10","High",8448]
["12.11","High",8449]
["12.12","High",8450]
["12.13","High",8451]
["12.14","High",8452]
["12.15","High",8453]
["12.16","High",8454]
["12.17","High",8455]
["12.18","High",8456]
["12.19","High",8457]
["12.2","High",8439]
["12.20","High",8458]
["12.21","High",8459]
["12.3","High",8441]
["12.4","High",8442]
["12.5","High",8443]
["12.6","High",8444]
["12.7","High",8445]
["12.8","High",8446]
["12.9","High",8447]
["12.99","High",8460]
["2.1","Very High",8296]
["2.1.9","Very High",11259]
["2.10","Medium",8304]
["2.11","Medium",8305]
["2.12","Low",8306]
["2.13","Low",8307]
["2.14","Low",8308]
["2.15","Low",8309]
["2.16","Medium",8310]
["2.2","Medium",8297]
["2.3","High",8295]
["2.4","Medium",8298]
["2.5","Medium",8299]
["2.6","Low",8300]
["2.7","High",8301]
["2.8","High",8302]
["2.9","Medium",8303]
["2.99","High",8311]
["3.1","High",8312]
["3.2","Very High",8313]
["3.3","High",8314]
["3.4","Low",8294]
["3.5","Medium",8315]
["3.6","High",8316]
["3.7","Very High",8317]
["3.8","Very High",8318]
["3.99","High",8319]
["4.1","High",8320]
["4.10","High",8329]
["4.11","Medium",8330]
["4.12","Very High",8331]
["4.13","Very High",8332]
["4.14","Very High",8333]
["4.15","Very High",8334]
["4.16","Very High",8335]
["4.17","Very High",8336]
["4.18","Very High",8337]
["4.19","Low",8338]
["4.2","Medium",8321]
["4.20","Very High",8339]
["4.21","High",8340]
["4.22","Low",8341]
["4.23","High",8342]
["4.24","High",8343]
["4.25","Low",8344]
["4.26","Low",8345]
["4.27","High",8346]
["4.3","Medium",8322]
["4.4","High",8323]
["4.5","Very High",8324]
["4.6","Medium",8325]
["4.7","High",8326]
["4.8","Medium",8327]
["4.9","Medium",8328]
["4.99","High",8347]
["5.1","Very High",8517]
["5.10","High",8526]
["5.11","Low",8527]
["5.12","Medium",8528]
["5.13","High",8529]
["5.14","Very High",8530]
["5.15","Medium",8531]
["5.16","Very High",8532]
["5.17","Very High",8533]
["5.18","High",8534]
["5.19","Medium",8535]
["5.2","Very High",8518]
["5.20","Medium",8536]
["5.21","Medium",8537]
["5.22","High",8539]
["5.23","Very High",8540]
["5.24","Very High",8541]
["5.25","Medium",8542]
["5.26","Medium",8543]
["5.27","Medium",8544]
["5.28","Very High",8545]
["5.29","High",8546]
["5.3","Low",8519]
["5.30","High",8547]
["5.31","High",8548]
["5.32","High",8549]
["5.33","High",8550]
["5.34","Low",8551]
["5.35","Medium",8552]
["5.36","Low",8553]
["5.37","Low",8554]
["5.38","High",8555]
["5.39","Very High",8556]
["5.4","High",8520]
["5.40","Very High",8557]
["5.41","Very High",8558]
["5.42","Medium",8559]
["5.43","High",8560]
["5.44","High",8561]
["5.45","Medium",8564]
["5.46","Medium",8565]
["5.47","Medium",8566]
["5.48","Medium",8567]
["5.5","Low",8521]
["5.6","Low",8522]
["5.7","Medium",8523]
["5.8","Medium",8524]
["5.9","Very High",8525]
["5.99","High",8568]
["6.1","Medium",8348]
["6.10","Low",8357]
["6.11","High",8358]
["6.12","Medium",8359]
["6.13","Low",8360]
["6.14","High",8361]
["6.15","High",8362]
["6.16","Very High",8363]
["6.17","Very High",8364]
["6.18","Medium",8365]
["6.19","Low",8366]
["6.2","High",8349]
["6.20","Medium",8367]
["6.21","High",8368]
["6.22","Medium",8369]
["6.3","Low",8350]
["6.4","High",8351]
["6.5","Medium",8352]
["6.6","Medium",8353]
["6.7","High",8354]
["6.8","High",8355]
["6.9","Low",8356]
["6.99","High",8370]
["7.1","High",8371]
["7.10","High",8380]
["7.11","High",8381]
["7.12","High",8382]
["7.13","Medium",8383]
["7.14","Medium",8384]
["7.15","High",8385]
["7.16","High",8386]
["7.17","High",8387]
["7.2","High",8372]
["7.3","Low",8373]
["7.4","Low",8374]
["7.5","Low",8375]
["7.6","Medium",8376]
["7.7","Low",8377]
["7.8","High",8378]
["7.9","High",8379]
["7.99","High",8388]
["8.1","Very High",8569]
["8.10","Very High",8578]
["8.100","Low",11227]
["8.101","Medium",11228]
["8.102","Low",11229]
["8.103","Low",11230]
["8.104","Low",11231]
["8.105","Medium",11232]
["8.106","Medium",11233]
["8.107","Low",11234]
["8.108","High",11235]
["8.109","Very High",11236]
["8.11","Medium",8579]
["8.110","High",11237]
["8.111","Medium",11238]
["8.112","High",11239]
["8.113","Medium",11240]
["8.114","Low",11241]
["8.115","High",11242]
["8.116","Medium",11243]
["8.117","Medium",11244]
["8.118","Medium",11245]
["8.119","High",11246]
["8.12","Medium",8580]
["8.120","High",11247]
["8.121","Medium",11248]
["8.122","High",11249]
["8.123","High",11250]
["8.124","Low",11251]
["8.125","High",11252]
["8.126","Medium",11253]
["8.127","Medium",11254]
["8.13","Medium",8581]
["8.14","Very High",8582]
["8.15","High",8583]
["8.16","Very High",8584]
["8.17","Low",8585]
["8.18","High",8586]
["8.19","High",8587]
["8.199","High",11255]
["8.2","Medium",8570]
["8.20","Medium",8588]
["8.21","High",8589]
["8.22","Very High",8590]
["8.23","Medium",8591]
["8.24","Medium",8592]
["8.25","Very High",8593]
["8.26","High",8594]
["8.27","Medium",8595]
["8.28","Medium",8596]
["8.29","High",8598]
["8.3","Very High",8571]
["8.30","High",8599]
["8.31","High",8600]
["8.32","Low",8601]
["8.33","Medium",8602]
["8.34","High",8603]
["8.35","Medium",8604]
["8.36","Medium",8605]
["8.37","High",8607]
["8.38","Medium",8608]
["8.39","Medium",8609]
["8.4","Medium",8572]
["8.40","High",8610]
["8.41","Medium",8611]
["8.42","Medium",8612]
["8.43","Very High",8613]
["8.44","High",8615]
["8.45","High",8616]
["8.46","Very High",8617]
["8.47","Very High",8618]
["8.48","Medium",8619]
["8.49","High",8620]
["8.5","Very High",8573]
["8.50","Medium",8621]
["8.51","Low",8622]
["8.52","Low",8623]
["8.53","Low",8624]
["8.54","High",8625]
["8.55","Low",11182]
["8.56","Medium",11183]
["8.57","Medium",11184]
["8.58","High",11185]
["8.59","High",11186]
["8.6","Medium",8574]
["8.60","High",11187]
["8.61","Medium",11188]
["8.62","Very High",11189]
["8.63","High",11190]
["8.64","Medium",11191]
["8.65","Low",11192]
["8.66","High",11193]
["8.67","High",11194]
["8.68","High",11195]
["8.69","Medium",11196]
["8.7","High",8575]
["8.70","Medium",11197]
["8.71","Very High",11198]
["8.72","Medium",11199]
["8.73","Medium",11200]
["8.74","High",11201]
["8.75","Medium",11202]
["8.76","Medium",11203]
["8.77","Medium",11204]
["8.78","Medium",11205]
["8.79","Medium",11206]
["8.8","Medium",8576]
["8.80","Medium",11207]
["8.81","Low",11208]
["8.82","Medium",11209]
["8.83","Low",11210]
["8.84","Low",11211]
["8.85","Medium",11212]
["8.86","Medium",11213]
["8.87","Medium",11214]
["8.88","Low",11215]
["8.89","High",11216]
["8.9","High",8577]
["8.90","High",11217]
["8.91","High",11218]
["8.92","Medium",11219]
["8.93","Low",11220]
["8.94","Low",11221]
["8.95","Medium",11222]
["8.96","Medium",11223]
["8.97","Low",11224]
["8.98","High",11225]
["8.99","Medium",11226]
["9.1","Low",8390]
["9.10","Medium",8399]
["9.11","Medium",8400]
["9.12","Medium",8401]
["9.13","Low",8402]
["9.14","Medium",8403]
["9.15","Medium",8404]
["9.16","High",8405]
["9.17","High",8406]
["9.18","Low",8407]
["9.19","Low",8408]
["9.2","Very High",8391]
["9.20","Medium",8409]
["9.21","Medium",8410]
["9.22","Low",8411]
["9.23","Low",8412]
["9.24","Medium",8413]
["9.25","Low",8414]
["9.26","Low",8415]
["9.27","Low",8416]
["9.28","Medium",8417]
["9.29","Low",8418]
["9.3","Very High",8392]
["9.4","High",8393]
["9.5","High",8394]
["9.6","Low",8395]
["9.7","Medium",8396]
["9.8","Medium",8397]
["9.9","Medium",8398]
["9.99","High",8419]

{"sheet":"Equipment_list","index":7,"n_rows":28,"n_cols":3,"rows_kept":28,"cut":false,"hidden":true,"merged":[]}
["TITLE","Equipment_list_description","ID"]
["Accommodation",null,12]
["Cargo Mach.",null,13]
["Critical Equip.",null,16]
["Deck - Machinery",null,18]
["Deck - Mooring Machinery",null,15]
["Deck - Pipe / Fittings",null,20]
["Documentation",null,21]
["E/R - Air Comp.",null,8]
["E/R - Aux. Engine",null,4]
["E/R - Aux. Mach.",null,7]
["E/R - Boiler",null,5]
["E/R - Main Engine",null,3]
["E/R - Pipes/ valves & fittings",null,9]
["E/R - Pumps",null,32]
["E/R - Purifier",null,6]
["Elect. Mach. & Equip.",null,10]
["Hull & Tanks",null,19]
["Inert Gas",null,14]
["LSA / FFA",null,17]
["Miscellaneous",null,22]
["Navigation - DGPS / EPFS / AIS",null,28]
["Navigation - ECDIS",null,25]
["Navigation - Echo Sounder / Speed Log",null,26]
["Navigation - GMDSS & Communication",null,23]
["Navigation - Others",null,11]
["Navigation - RADAR",null,24]
["Navigation - VDR / BNWAS",null,30]

{"sheet":"PSC_MOU","index":8,"n_rows":11,"n_cols":3,"rows_kept":11,"cut":false,"hidden":true,"merged":[]}
["TITLE","PSC_MOU_description","ID"]
["Asia and the Pacific",null,2]
["Caribbean",null,4]
["Europe and the North Atlantic",null,1]
["Latin America",null,3]
["The Black Sea region",null,6]
["The Indian Ocean",null,8]
["The Mediterranean",null,7]
["The Riyadh MoU",null,9]
["USCG",null,10]
["West and Central Africa",null,5]

{"sheet":"Inspection_type","index":9,"n_rows":13,"n_cols":2,"rows_kept":13,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Bunkering Audit",14]
["Cargo Audit",17]
["Engineering Audit",16]
["ISM Audit",2]
["ISPS Audit",3]
["IT Audit",10]
["MLC Audit",1]
["Mooring Audit",9]
["Nav Audit / Verification",8]
["Onboard Training",18]
["Ship Staff Insp.",15]
["Suptd. Insp.",13]

{"sheet":"Deficiency_Cause","index":10,"n_rows":8,"n_cols":3,"rows_kept":8,"cut":false,"hidden":true,"merged":[]}
["TITLE","Deficiency_Cause_description","ID"]
["Behaviour Based",null,1]
["Equipment Related",null,4]
["External Factors",null,5]
["Human Error",null,7]
["Inappropriate Procedure",null,8]
["Industry Issue",null,6]
["Knowledge Based",null,3]

{"sheet":"Observer_code","index":11,"n_rows":3,"n_cols":3,"rows_kept":3,"cut":false,"hidden":true,"merged":[]}
["TITLE","Observer_code_description","ID"]
["Owner / Marine / Tech. Suptd.",null,3]
["Ship Staff",null,2]

{"sheet":"Status_code","index":12,"n_rows":6,"n_cols":3,"rows_kept":6,"cut":false,"hidden":true,"merged":[]}
["TITLE","Status_code_description","ID"]
["Completed",null,6]
["Deferred to D D",null,5]
["In progress",null,3]
["Not Started",null,2]
["Waiting spare",null,4]

{"sheet":"PSC_ref_no","index":13,"n_rows":19,"n_cols":2,"rows_kept":19,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Alarms",9]
["Cargo operations including equipment",7]
["Certificates & Documentation",2]
["Dangerous Goods",13]
["Emergency Systems",5]
["Fire safety",8]
["ISM",16]
["ISPS",17]
["Life saving appliances",12]
["MLC, 2006",18]
["Other",19]
["Pollution Prevention",15]
["Propulsion and auxiliary machinery",14]
["Radio communication",6]
["Safety of Navigation",11]
["Structural condition",3]
["Water/Weathertight condition",4]
["Working and Living Conditions",10]

{"sheet":"Risk_value_of_obs","index":14,"n_rows":1,"n_cols":2,"rows_kept":1,"cut":false,"hidden":true,"merged":[]}
["Risk Value of observation","ID"]

{"sheet":"Year","index":15,"n_rows":18,"n_cols":1,"rows_kept":18,"cut":false,"hidden":true,"merged":[]}
["Year"]
[2014]
[2015]
[2016]
[2017]
[2018]
[2019]
[2020]
[2021]
[2022]
[2023]
[2024]
[2025]
[2026]
[2027]
[2028]
[2029]
[2030]

{"sheet":"Month","index":16,"n_rows":13,"n_cols":1,"rows_kept":13,"cut":false,"hidden":true,"merged":[]}
["Month"]
["Jan"]
["Feb"]
["Mar"]
["Apr"]
["May"]
["Jun"]
["Jul"]
["Aug"]
["Sep"]
["Oct"]
["Nov"]
["Dec"]

{"sheet":"Date_","index":17,"n_rows":32,"n_cols":1,"rows_kept":32,"cut":false,"hidden":true,"merged":[]}
["Date"]
["01"]
["02"]
["03"]
["04"]
["05"]
["06"]
["07"]
["08"]
["09"]
[10]
[11]
[12]
[13]
[14]
[15]
[16]
[17]
[18]
[19]
[20]
[21]
[22]
[23]
[24]
[25]
[26]
[27]
[28]
[29]
[30]
[31]

{"sheet":"Sheet1","index":18,"n_rows":24,"n_cols":6,"rows_kept":24,"cut":false,"hidden":true,"merged":[]}
[]
[null,"ID","E",null,"Date Recorded",1]
[null,"UNIQUE ID","F",null,"Type of Deficiency",2]
[1,"Date Recorded","G",null,"Observer code",3]
["ignore","Vessel Type","H",null,"Type of Inspection",4]
[null,"Internal / External","I",null,"Description of Deficiency",5]
[null,"Drydock","J",null,"Equipment Categories",6]
[null,"Information Sharing","K",null,"Area of Observation",7]
[null,"Critical_item","L",null,"Deficiency Cause",8]
[null,"Deficiency Type","M",null,"VIQ Ref Number",9]
[null,"Deficiency Cause","N",null,"Risk Value of Obs",10]
[null,"Inspection Type","O",null,"PSC Ref Number",11]
[null,"Equipments","P",null,"PSC MOU ID",12]
[null,"VIQ Reference Number","Q",null,"Action Taken or Required",13]
[null,"Risk Value of the observation","R",null,"Target Date",14]
[null,"PSC Reference Number","S",null,"PO Ref No.",15]
[null,"PSC MOU","T",null,"Status Code",16]
[null,"Observer Code","U",null,"Date Completed",17]
[null,"Target Date","V",null,"Drydock",18]
[null,"Status Code","W",null,"Info Sharing",19]
[null,"Description of Deficiency","X",null,"Critical Item Flag",20]
[null,"Action taken / required","Y",null,"Audit Type",21]
[null,"PO ref no","Z"]
[null,"Date completed","AA"]

{"sheet":"Ship_information","index":19,"n_rows":2,"n_cols":3,"rows_kept":2,"cut":false,"hidden":true,"merged":[]}
["Ship_ID","Ship_Name","FILE_NAME"]
["22","DHT FALCON (06-08-2021)","22_1628242979936.xlsm"]

{"sheet":"External_Deficiency_type","index":20,"n_rows":5,"n_cols":3,"rows_kept":5,"cut":false,"hidden":true,"merged":[]}
["TITLE","Type of deficiency_description","ID"]
["Condn of Class / Memo",null,5]
["Defect",null,1]
["Non Conformity",null,2]
["Observation",null,3]

{"sheet":"External_Inspection_type","index":21,"n_rows":11,"n_cols":2,"rows_kept":11,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Cargo Audit",17]
["Flag State Insp.",5]
["ISM Audit",2]
["ISPS Audit",3]
["MLC Audit",1]
["Nav Audit / Verification",8]
["OM Insp. (Eg. SIRE / CDI etc.)",6]
["Others (Eg. Insurance etc.)",12]
["PSC Inspection",4]
["Terminal Insp.",11]

{"sheet":"External_Observer_code","index":22,"n_rows":7,"n_cols":3,"rows_kept":7,"cut":false,"hidden":true,"merged":[]}
["TITLE","Observer_code_description","ID"]
["Class Surveyor",null,4]
["FSC Inspector",null,5]
["Others (Eg. Insurance etc.)",null,9]
["PSC Insp.",null,6]
["SIRE / CDI Insp.",null,8]
["Terminal Insp.",null,7]

{"sheet":"Sheet Version","index":23,"n_rows":2,"n_cols":2,"rows_kept":2,"cut":false,"hidden":true,"merged":[]}
["Version","Title"]
["2.0","Version 2.0"]