{"text_format":"1","workbook":"xlsx","n_sheets":24,"sheets":["Mainsheet","Completed","Calc","Areaofobs","Vessel_type","Deficiency_type","VIQrefno","Equipment_list","PSC_MOU","Inspection_type","Deficiency_Cause","Observer_code","Status_code","PSC_ref_no","Risk_value_of_obs","Year","Month","Date_","Sheet1","Ship_information","External_Deficiency_type","External_Inspection_type","External_Observer_code","Sheet Version"],"not_rendered":{"charts":0,"images":6,"macros":1,"external_links":0,"defined_names":12,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Mainsheet","index":0,"n_rows":22,"n_cols":28,"rows_kept":22,"cut":false,"hidden":false,"merged":[[10,8,10,9],[10,12,10,13],[12,6,12,27],[8,6,8,27]]}
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,"Defect - Damage Monitoring Sheet"]
[]
[null,null,null,null,null,null,null,"Date of Report","29-Apr-2021",null,null,"Ship Name","EAGLE BAY (28-02-2021)"]
[]
[null,null,null,null,null,null,"VERSION : 2.0"]
[]
[]
[]
[null,null,null,null,"ID","UNIQUE ID","Date Recorded","Type of Deficiency","Observer code","Type of Inspection","Description of Deficiency","Equipment Categories","Area of Observation","Deficiency Cause","VIQ Ref Number","Risk Value of Obs","PSC Ref Number","PSC MOU ID","Action Taken or Required","Target Date","PO Ref No.","Status Code","Date Completed","Drydock","Info Sharing","Critical Item","Audit Type","Superintendent Remarks"]
[null,null,null,null,null,"52_01/05/2021 18:28:29","2021-01-05","Observation","Owner / Marine / Tech. Suptd.","Ship Staff Insp.","SVDR back up cannot be replayed onboard as due to playbacksoftware not available","Navigation - VDR / BNWAS","Navigation","Equipment Related",4.1100000000000003,"Medium","Not Applicable","Not Applicable","Liaise with makers to obtain playback software.","2021-07-30",null,"In progress",null,"No",null,null,"Internal"]
[null,null,null,null,null,"52_01/05/2021 18:48:11","2021-02-03","Observation","Ship Staff","Ship Staff Insp.","Port anchor chain 5th common link stud in the 1st shackle is missing. Port side anchor chain 8th common link stud in the 1st shackle has bent slightly.","Deck - Mooring Machinery","Mooring","Equipment Related",9.1999999999999993,"Medium","Not Applicable","Not Applicable","Hotwork is required to the job, awaiting gas free condition opportunity to do same.","2021-10-30",null,"Not Started",null,"No",null,null,"Internal"]
[null,null,null,null,null,"52_5/8/2021 10:03:18 AM","2021-04-05","Defect","Ship Staff","Ship Staff Insp.","Fresh water ejector pump drawing more current during operation.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related",null,null,"Not Applicable","Not Applicable","Need ejector pump spare ","2021-07-15",null,"Waiting spare",null,"No",null,null,"Internal"]
[null,null,null,null,null,"52_5/8/2021 9:53:06 AM","2021-07-27","Defect","Ship Staff","Ship Staff Insp.","Sewage blower motor winding  found damage.Need motor renewal.","E/R - Aux. Mach.","MARPOL Related","Equipment Related",6.3,"Low","Not Applicable","Not Applicable","Requisition raised for new motor","2021-08-15","EBAY210134","Waiting spare",null,"No",null,null,"Internal"]
[null,null,null,null,null,"52_05/08/2021 19:25:57","2021-07-29","Defect","Ship Staff","Ship Staff Insp.","SOPEP pump inoperational due to worn out diaphragm.","Miscellaneous","MARPOL Related","Equipment Related",6.3,"Low","Not Applicable","Not Applicable","Awaiting spare to replace same.","2021-10-31","EBAY210133","Waiting spare",null,"No",null,null,"Internal"]

{"sheet":"Completed","index":1,"n_rows":209,"n_cols":28,"rows_kept":209,"cut":false,"hidden":false,"merged":[[10,8,10,9],[10,12,10,13],[12,6,12,27],[8,6,8,27]]}
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,"Defect - Damage Monitoring Sheet"]
[]
[null,null,null,null,null,null,null,"Date of Report","29-Apr-2021",null,null,"Ship Name","EAGLE BAY (28-02-2021)"]
[]
[null,null,null,null,null,null,"VERSION : 2.0"]
[]
[]
[]
[null,null,null,null,"ID","UNIQUE ID","Date Recorded","Type of Deficiency","Observer code","Type of Inspection","Description of Deficiency","Equipment Categories","Area of Observation","Deficiency Cause","VIQ Ref Number","Risk Value of Obs","PSC Ref Number","PSC MOU ID","Action Taken or Required","Target Date","PO Ref No.","Status Code","Date Completed","Drydock","Info Sharing","Critical Item","Audit Type","Superintendent Remarks"]
[null,null,null,null,4901,"52_25/10/2019 8:40:52 AM","2019-01-15","Defect","Ship Staff","Ship Staff Insp.","FUEL OIL TEMP. CONTROLLER FOR ME & AE'S NOT FUNCTIONING PROPERLY AND NEED TO BE ADJUSTED MANUALLY. VISCOTHERM SENSOR WAS FOUND NOT GIVING SIGNAL TO INTERFACE BOX. AFTER INSTALLING NEW SENSOR THE TEMPERATURE CONTROLLER IS STILL NOT RESPONDING. AFTER INVESTIGATION FOUND THAT INTERFACE BOX PCB IS DAMAGED. ALSO THE ACTUATOR FOR TEMPERATURE CONTROL VALVE IS SLUGGISH.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","repalced with new spares","2019-12-31","","Completed","2020-01-04","No","No","No","Internal","Noted."]
[null,null,null,null,4902,"52_25/10/2019 8:54:47 AM","2019-01-16","Defect","Ship Staff","Ship Staff Insp.","AE INLET/OUTLET FUEL OIL FLOWMETER FAULTY","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","OVERHAULED WITH OLD SPARE FROM ANOTHER METER","2019-12-31","","Completed","2020-03-09","No","No","No","Internal","Noted. Follow up in progress."]
[null,null,null,null,9295,"52_23/12/2019 9:36:38 AM","2019-02-26","Non Conformity","Owner / Marine / Tech. Suptd.","ISM Audit","ISM Audit - Swivel for Fixed Monitor located on the main deck swivel found frozen. Resulting in the monitor being very difficult to turn.","LSA / FFA","Safety / LSA / FFA","Behaviour Based,Industry Issue,Knowledge Based","5.35","Medium","","","Foam Monitor greased and freed","2019-05-19","","Completed","2019-03-05","No","No","No","Internal"]
[null,null,null,null,9296,"52_23/12/2019 11:20:35 AM","2019-02-26","Non Conformity","Owner / Marine / Tech. Suptd.","ISM Audit","ISM Audit - Combustible material like wooden support, wooden label etc located inside oxy/acetylene room","Miscellaneous","ISM Related","Behaviour Based,Knowledge Based","5.26","Medium","","","Combustible material were immediately removed from oxygen/acetylene room. Oxygen/acetylene room to be checked regularly/saturday safety rounds for cleanliness. Discussed in safety meeting and crew briefed not to store any combustible material in O2/Acetylene room.","2019-05-19","","Completed","2019-02-27","No","No","No","Internal"]
[null,null,null,null,9297,"52_23/12/2019 11:29:58 AM","2019-02-26","Observation","Owner / Marine / Tech. Suptd.","ISM Audit","ISM Audit - No. 1 Deck Seal Pump Guage not operational","Inert Gas","Cargo / Ballast Systems","Behaviour Based,Industry Issue,Knowledge Based","8.25","Medium","","","Deck seal pump gauge replaced. Regular checks of all pressure gauges to be included in PMS.","2019-05-19","","Completed","2019-03-01","No","No","No","Internal"]
[null,null,null,null,9298,"52_23/12/2019 11:40:53 AM","2019-02-26","Observation","Owner / Marine / Tech. Suptd.","ISM Audit","ISM Audit - Total 5 Emergency and 2 normal lights not working around accommodation block","Elect. Mach. & Equip.","ISM Related","Behaviour Based,Equipment Related,External Factors,Industry Issue,Knowledge Based","11.11","Very High","","","Emergency lights were replace immediately. All emergency lights to be checked during saturday safety routine.","2019-05-19","","Completed","2019-02-28","No","No","No","Internal"]
[null,null,null,null,9299,"52_23/12/2019 11:51:16 AM","2019-02-26","Observation","Owner / Marine / Tech. Suptd.","ISM Audit","ISM Audit - Incorect Fire Plan IMO Symbol in Use","LSA / FFA","ISM Related","Knowledge Based","5.37","Low","","","New IMO symbol for fire plan was stencilled","2019-05-19","","Completed","2019-02-28","No","No","No","Internal"]
[null,null,null,null,9300,"52_23/12/2019 2:52:23 PM","2019-02-26","Observation","Owner / Marine / Tech. Suptd.","ISM Audit","ISM Audit - Locking Plate Missing from 1 Chain Block kept in midship store stbd side","Miscellaneous","ISM Related","Behaviour Based,Industry Issue,Knowledge Based","10.28","Low","","","Locking Plate Fabricated. Inspection of loose gears to be carried out as per PMS","2019-05-19","","Completed","2019-03-10","No","No","No","Internal"]
[null,null,null,null,9301,"52_23/12/2019 2:59:33 PM","2019-02-26","Observation","Owner / Marine / Tech. Suptd.","ISPS Audit","ISPS Audit - Securing arrangement for CITADEL to be fabricated.","Miscellaneous","ISPS Related","Behaviour Based,Industry Issue,Knowledge Based","7.4","Low","","","Citadel dook locking plate fabricated. As soon as vessel is takeover by management, Citadel arrangement to be audited and corrected as necessary.","2019-02-28","","Completed","2019-02-28","No","No","No","Internal"]
[null,null,null,null,9302,"52_23/12/2019 3:04:56 PM","2019-02-26","Observation","Owner / Marine / Tech. Suptd.","MLC Audit","MLC Audit - Weekly food menu to be prepared and displayed in both mess rooms","Miscellaneous","MLC Related","Behaviour Based,Industry Issue,Knowledge Based","","","","","Weekly menu for officer and crew messroom was posted.Ch. Cook will be briefed in Familiarisation upon joining the vessel to post the weekly menu in messrooms.","2019-05-19","","Completed","2019-02-27","No","No","No","Internal"]
[null,null,null,null,9303,"52_23/12/2019 3:09:37 PM","2019-02-26","Observation","Owner / Marine / Tech. Suptd.","Nav Audit / Verification","Navigation Audit - Weekly entries as per SOLAS Ch 3 regulation 20.6 to be made in deck log book","Miscellaneous","Navigation","Behaviour Based,Industry Issue,Knowledge Based","","","","","Entries as per SOLAS made on weekly basis. Deck logbook to be verified by master and chief officer daily.","2019-05-19","","Completed","2019-03-02","No","No","No","Internal"]
[null,null,null,null,9304,"52_23/12/2019 3:13:28 PM","2019-02-26","Observation","Owner / Marine / Tech. Suptd.","Nav Audit / Verification","Navigation Audit - Inventory of bridge equipment spares to be updated","Navigation - Others","Navigation","Behaviour Based,Industry Issue,Knowledge Based","10.13","Very High","","","Inventory updated. Vessel taken over recently. ","2019-05-19","","Completed","2019-02-28","No","No","No","Internal"]
[null,null,null,null,9305,"52_23/12/2019 3:17:07 PM","2019-02-26","Observation","Owner / Marine / Tech. Suptd.","Nav Audit / Verification","Navigation Audit - Position Verification Interval marked on ECDIS not complied.","Navigation - ECDIS","Navigation","Behaviour Based,Industry Issue,Knowledge Based","4.17","Very High","","","Position verification as per PPI followed. All OOW briefed to comply with PPI.","2019-05-19","","Completed","2019-02-27","No","No","No","Internal"]
[null,null,null,null,9306,"52_23/12/2019 3:21:21 PM","2019-02-26","Observation","Owner / Marine / Tech. Suptd.","Mooring Audit","Mooring Audit - Striking direction arrow for releasing bitter end to be clearly marked in the vicinity of the bitter end.","Miscellaneous","Mooring","Industry Issue,Knowledge Based","9.22","Low","","","Instruction indicating striking direction to release bitter end was posted near bitter end. Stencils to be checked regularly.","2019-05-19","","Completed","2019-02-28","No","No","No","Internal"]
[null,null,null,null,9307,"52_23/12/2019 3:40:28 PM","2019-02-26","Observation","Owner / Marine / Tech. Suptd.","Mooring Audit","Mooring Audit - Working areas around mooring winchs on main deck to be covered with anti-skid coatings","Miscellaneous","Mooring","Behaviour Based,Industry Issue,Knowledge Based","9.13","Low","","","Anti-skid paint was applied near mooring winches. Regular deck rounds to be taken.","2019-05-19","","Completed","2019-03-07","No","No","No","Internal"]
[null,null,null,null,9308,"52_23/12/2019 3:58:28 PM","2019-02-26","Observation","Owner / Marine / Tech. Suptd.","Others (Eg. Insurance etc.)","Cargo Audit - No records available for continuity test of portable tank cleaning hoses.","Miscellaneous","Cargo / Ballast Systems","Behaviour Based,Industry Issue,Knowledge Based","8.45","High","","","Continuity test of all portable hoses carried out.Continuity test of postable cargo hoses included in PMS and will be checked as per schedule.","2019-05-19","","Completed","2019-03-04","No","No","No","Internal"]
[null,null,null,null,9309,"52_23/12/2019 4:01:46 PM","2019-02-26","Observation","Owner / Marine / Tech. Suptd.","Others (Eg. Insurance etc.)","Cargo Audit - Port emergency contact list missing contact details for Terminal/H&M insurance","Documentation","Cargo / Ballast Systems","Behaviour Based,Industry Issue,Knowledge Based","","","","","Port Contact List was amended. Officer designated briefed.","2019-05-19","","Completed","2019-02-26","No","No","No","Internal"]
[null,null,null,null,9310,"52_23/12/2019 4:07:23 PM","2019-02-26","Observation","Owner / Marine / Tech. Suptd.","Others (Eg. Insurance etc.)","Cargo Audit - \"During loading opeartions ensure next set of tank valve are open before closing any tank valves\" notice to be posted.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Behaviour Based,Industry Issue,Knowledge Based","","","","","Poster posted in CCR. Posters in CCR to be posted as per SMS.","2019-05-19","","Completed","2019-03-13","No","No","No","Internal"]
[null,null,null,null,4903,"52_25/10/2019 9:17:18 AM","2019-02-27","Defect","Ship Staff","Ship Staff Insp.","STBD SIDE BALLAST PUMP DISCHARGE PRESSURE READING INCORRECT","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.23","Medium","","","repalced sensor with new spares","2019-12-31","","Completed","2020-01-26","No","No","No","Internal"]
[null,null,null,null,9311,"52_23/12/2019 4:13:27 PM","2019-03-04","Observation","Ship Staff","Nav Audit / Verification","Celestial observation were not being practiced and obtained since take over of the vessel.","Miscellaneous","Navigation","Behaviour Based,Industry Issue,Knowledge Based","","","","","Celestial observation were taken by OOW. OOW were briefed to take celestial observation frequently and at least once during voyage.","2019-04-04","","Completed","2019-03-23","No","No","No","Internal"]
[null,null,null,null,9312,"52_23/12/2019 4:26:29 PM","2019-03-04","Observation","Ship Staff","Nav Audit / Verification","Weather Faxes were not obtained using Facsimile recorder. Weather reports were only monitored using software based system - SPOS","Navigation - Others","Navigation","Behaviour Based,Industry Issue,Knowledge Based","","","","","Weather Facimile was tuned and weather fac taken. OOW were briefed to take wather Fax regularly","2019-04-04","","Completed","2019-03-23","No","No","No","Internal"]
[null,null,null,null,9313,"52_23/12/2019 5:35:53 PM","2019-03-04","Observation","Ship Staff","Nav Audit / Verification","Manual Radar Plotting Techniques were not being practiced","Navigation - RADAR","Navigation","Behaviour Based,Industry Issue,Knowledge Based","","","","","Radar plotting wre carried out once a watch as per availability of targets. OOW were breifed to carry out Radar Plotting regularly.","2019-04-04","","Completed","2019-03-23","No","No","No","Internal"]
[null,null,null,null,10437,"52_2/10/2020 11:21:37 AM","2019-05-23","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","GAUGES (PRESSURE GAUGES, THERMOMETERS) ON ALL MACHINERIES ON BOARD TO QUANTIFY, LIST AND ENSURE EVERY GAUGE IS WORKING AS PER OUR COMPANY POLICY. PLEASE SEND LIST OF GAUGES, THEIR WORKING STATUS EVERY MONTH. REQUISITION TO BE RAISED FOR FAULTY GAUGES.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","In Progress. Awaiting a few gauges in supply.\n\n","2019-06-22","","Completed","2019-06-15","No","No","No","Internal"]
[null,null,null,null,10438,"52_2/10/2020 11:33:53 AM","2019-05-23","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","EACH AND EVRY VALVE ON DECK OF CARGO LINES, HYDRAULIC LINES, STEAM LINES, FIRE LINES, FOAM LINE TO CHECK FOR OPERATION AND ENSURE OPERATIONABILITY OF EACH ONE.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","","","","","All valves in operational state","2019-07-23","","Completed","2019-07-15","No","No","No","Internal"]
[null,null,null,null,10439,"52_2/10/2020 11:44:01 AM","2019-05-23","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","HEATING COILS TO PESSURE TEST. ALSO UPGRADE COSMETICALLY.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","","","","","Heating coil pressure testing carried out","2019-06-30","","Completed","2019-06-27","No","No","No","Internal"]
[null,null,null,null,10440,"52_2/10/2020 11:47:27 AM","2019-05-23","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","BALLAST TANK VENTS: EACH ONE TO OPEN, INSPECT AND CARRY OUT REQUIRED MAINTENANCE.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","","","","","Completed ","2019-07-22","","Completed","2019-06-13","No","No","No","Internal"]
[null,null,null,null,10441,"52_2/10/2020 11:49:34 AM","2019-05-23","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","INCINERATOR REFRACTORY CONDITION MONITORING IS CONTINUOUS PHENOMENON AND SHOULD BECOMPLIED. ENSURE COOLING HOLES DOES EXIST ALL THE TIME. KEEP SOME STOCK OF REFRACTORY ALWAYS.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Incinerator refractory inspected regularly. ","2019-06-23","","Completed","2019-06-22","No","No","No","Internal"]
[null,null,null,null,10442,"52_2/10/2020 11:51:33 AM","2019-05-23","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ME UNIT #3 DECARB IS DUE, TO COMPLETE IT AS SOON AS OPPORTUNITY ARISES.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Unit no 3 decard completed and replaced the pistion rings.","2019-06-23","","Completed","2019-06-01","No","No","No","Internal"]
[null,null,null,null,10443,"52_2/10/2020 11:53:37 AM","2019-05-23","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","FRAMO SERVICE TANK LEVEL/SOUNDING LOG TO MAINTAIN. TO ORDER LEVEL SENSOR TO REPLACE DEFECTIVE SENSOR.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","New spares received and replaced ","2019-06-23","","Completed","2019-06-06","No","No","No","Internal"]
[null,null,null,null,10444,"52_2/10/2020 12:03:21 PM","2019-05-23","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","RUSTED AND THINNED DOWN GRATINGS ON CAT WALK ON DECK TO IDENTIFY AND RAISE REQUISITION FOR GRATINGS FOR REPLACEMENT. ","Deck - Pipe / Fittings","General Appearance","Equipment Related","","","","","Derusting Completed","2019-08-23","","Completed","2019-08-15","No","No","No","Internal"]
[null,null,null,null,10445,"52_2/10/2020 11:31:12 AM","2019-05-23","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","HOSE HANDLING CRANE HOSES TO INSPECT CLOSELY AND RENEW WORN OUT ONES. GREASING POINTS OF CRANE TO IDENTIFY, PAINT AND ENSURE REGULAR GREASING IS DONE.","Deck - Machinery","Eng. / Strg. Comp.","Equipment Related","","","","","Completed","2019-06-30","","Completed","2019-06-30","No","No","No","Internal"]
[null,null,null,null,4900,"52_25/10/2019 9:38:30 AM","2019-06-15","Defect","Ship Staff","Ship Staff Insp.","ONE UTI SHOWING ERRATIC ULLAGE AND TEMP READINGS","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.12","Medium","","","UTI received back after calibration","2019-12-31","","Completed","2019-12-10","No","No","No","Internal"]
[null,null,null,null,4905,"52_25/10/2019 9:34:52 AM","2019-06-15","Defect","Ship Staff","Ship Staff Insp.","MIDSHIP DRIP TRAY WIDEN PUMP NOT WORKING","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","6.6","Medium","","","CHANGED WITH NEW PUMP","2020-03-30","","Completed","2020-03-16","No","No","No","Internal"]
[null,null,null,null,4906,"52_25/10/2019 9:44:45 AM","2019-06-22","Defect","Ship Staff","Ship Staff Insp.","DECK FOAM STORAGE TANK MID-CONNECTOR CORRODED AND DAMAGED","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.36","Low","","","TEMPORARY REPAIR DONE ON THE CONNECTORS AND IN USE. RO RAISED FOR NEW CONNECTOR: EBAY190126.\n\nRENEWED THE GAUGE GLASS WITH NREW SPARE GAUGE GLASS ","2020-07-31","EBAY200092","Completed","2020-07-13","No","No","No","Internal","ORDERED FOAM STORAGE TANK COMPLETE GAUGE GLASS UNDER PO EBAY200092, SPARES CONNECTED , PLEASE UPDATE THE STATUS."]
[null,null,null,null,4907,"52_25/10/2019 9:51:18 AM","2019-07-08","Defect","Ship Staff","Ship Staff Insp.","4P WBT, 4S WBT, 5P WBT, SLOP P EMERGENCY HYDRAULIC PUMP CONNECTION POINTS LEAKING","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.11","Medium","","","Leaking connectors renewed with spares received.","2019-12-31","EBAY190190","Completed","2019-12-31","No","No","No","Internal"]
[null,null,null,null,4909,"52_25/10/2019 10:43:21 AM","2019-07-22","Defect","Ship Staff","Ship Staff Insp.","PORT SIDE BALLAST PUMP DISCHARGE PRESSURE READING INCORRECT","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.23","Medium","","","replaced with new sensor","2019-12-31","","Completed","2020-01-26","No","No","No","Internal","Noted"]
[null,null,null,null,9743,"52_15/1/2020 1:17:58 AM","2019-08-02","Observation","Owner / Marine / Tech. Suptd.","Nav Audit / Verification","Security level was not mentioned in the passage plan for each leg","Navigation - Others","Navigation","Knowledge Based","7.8","High","","","Immediately advised to Nav. Officer to put security level in each leg in remarks column in 12.01.34.022.01 Passage Plan Sheet A. Training carried out to all deck officer.","2019-08-15","","Completed","2019-08-03","No","No","No","Internal"]
[null,null,null,null,4910,"52_25/10/2019 10:50:27 AM","2019-08-18","Defect","Ship Staff","Ship Staff Insp.","STEERING GEAR SYSTEM PHASE MONITORING RELAY NON OPERATIONAL AND NEED TO REPLACE THE RELAY","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","RO RAISED FOR RELAY. EBAY190150","2019-12-31","","Completed","2019-12-18","No","No","No","Internal"]
[null,null,null,null,4911,"52_25/10/2019 10:59:33 AM","2019-08-18","Defect","Ship Staff","Ship Staff Insp.","MAIN DECK AND ENGINE ROOM LIGHT FITTINGS ARE DETERIORATING DUE TO AGE AND HIGH TEMPERATURE. CRACKS ARE BEING OBSERVED. NEED TO REPLACE THE FITTINGS","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","11.11","Very High","","","REPLACED WITH NEW SPARES ","2020-01-31","","Completed","2020-02-26","No","No","No","Internal","Noted"]
[null,null,null,null,9744,"52_15/1/2020 1:59:21 AM","2019-08-20","Non Conformity","Ship Staff","Ship Staff Insp.","During wet round found that midship store extinguisher not secured properly in it's place","LSA / FFA","Safety / LSA / FFA","Behaviour Based,Industry Issue,Knowledge Based","5.42","Medium","","","Immediately secured and training/briefing given to all crew.","2019-08-21","","Completed","2019-08-21","No","No","No","Internal"]
[null,null,null,null,9316,"52_25/12/2019 8:48:19 AM","2019-09-08","Defect","Ship Staff","Ship Staff Insp.","2 nos. 3-way ball valve for emergency operation of  stbd Ballast seachest and overboard valves wasted and broken. ","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.11","Medium","","","2nos. 3 way ball valves renewed.","2019-12-31","EBAY190172","Completed","2019-12-24","No","No","No","Internal"]
[null,null,null,null,4916,"52_25/10/2019 2:32:37 PM","2019-09-11","Defect","Ship Staff","Ship Staff Insp.","5P CARGO VALVE NOT OPERATIONAL FROM CCR, THE CHANNEL OF OUTPUT CARD IS NOT OPERATIONAL","Elect. Mach. & Equip.","Cargo / Ballast Systems","Equipment Related","8.11","Medium","","","Defect rectified.","2019-12-31","EBAY190175","Completed","2019-11-25","No","No","No","Internal"]
[null,null,null,null,4913,"52_25/10/2019 2:52:14 PM","2019-09-15","Defect","Ship Staff","Ship Staff Insp.","EPIRB HOLDING BRACKET TO BE RENEWED","Critical Equip.","Safety / LSA / FFA","Equipment Related","4.23","High","","","new bracket installed","2020-05-31","EBAY200111","Completed","2020-04-26","No","No","No","Internal","NEW EPIRB HOLDING BRACKET ORDERED, PO NO 200111 AND WILL BE CONNECTED ON BOARD ONCE READY. PLEASE ADVICE PRESENT STATUS; WHETHER IT IS RENEWED.                                      (ORIGINAL BRACKET WAS NOT ALSO BAD)."]
[null,null,null,null,4915,"52_25/10/2019 8:55:06 PM","2019-09-15","Defect","Ship Staff","Ship Staff Insp.","HOSES FOR EMERGENCY HAND PUMP TO OPERATE VALVES ARE BROKEN. ","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.11","Medium","","","Hoses and pressure gauges renewed.","2019-12-31","EBAY190172","Completed","2019-12-16","No","No","No","Internal"]
[null,null,null,null,4918,"52_25/10/2019 9:08:00 PM","2019-09-15","Defect","Ship Staff","Ship Staff Insp.","GRATINGS ON CATWALK AND UNDER MANIFOLD ARE IN BAD AND WASTED CONDITION. ","Miscellaneous","General Appearance","Equipment Related,External Factors","11.4","Very High","","","NEW SPARES RECIEVED AND RENEWED","2020-03-29","EBAY200051","Completed","2020-03-22","No","No","No","Internal","Noted. Send us the action plan."]
[null,null,null,null,9314,"52_23/12/2019 5:52:26 PM","2019-09-26","Non Conformity","Ship Staff","Ship Staff Insp.","During daily rounds in forepeak store it was found that two in no. receptacles foundationwas broken","Elect. Mach. & Equip.","General Appearance","Behaviour Based,Equipment Related,External Factors,Industry Issue,Knowledge Based","10.37","Medium","","","Requisition raised for receptacles EBAY190184. As a temporary measure receptacles connection wire isolated.All crew member were trained and explained the consequences of negligent behaiour towards electrical fittings. Also if some equipment is damages immediately it must be reported to the concerned officer. Required spare received on 09 Dec 2019 and renewed on 21 Dec 2019.","2019-12-30","UNDER EBAY190184 ITEM 7","Completed","2019-12-21","No","No","No","Internal"]
[null,null,null,null,7422,"52_15-11-2019 14:44:52","2019-10-20","Defect","Ship Staff","Ship Staff Insp.","IG TRANSMITTER BOX ON MAINDECK IN WASTED CONDITION","Inert Gas","Cargo / Ballast Systems","Equipment Related","8.3","Medium","","","TO BE FABRICATED AND RENEWED","2019-10-27","","Completed","2019-10-25","No","No","No","Internal"]
[null,null,null,null,4917,"52_25/10/2019 2:43:16 PM","2019-10-29","Non Conformity","Ship Staff","Ship Staff Insp.","FIRE DETECTION SYSTEM, 3 MANUAL CALL POINTS ON UPPER DECK PORT SIDE ENTRANCE (A27), STB'D SIDE UPPER DECK ENTRANCE (A34) AND A-DECK PORT SIDE ENTRANCE (A23) ARE NOT OPERATIONAL","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.35","Medium","","","NEED TO REPLACE MCP. RO RAISED. EBAY190180. RECEIVED SPARE IN BALBOA ON 09 DEC 2019 AND RENEWED ON 21 DEC 2019.","2019-12-31","","Completed","2019-12-21","No","No","No","Internal"]
[null,null,null,null,7425,"52_15/11/2019 15:48:43","2019-11-01","Defect","Ship Staff","Ship Staff Insp.","ACS controller for No.1 AC faulty","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Repaired the ACS controller and AC#1 tried out. Found working satisfactorily.","2019-11-30","","Completed","2019-11-03","No","No","No","Internal"]
[null,null,null,null,7423,"52_15-11-2019 14:54:11","2019-11-02","Defect","Ship Staff","Ship Staff Insp.","PORT SIDE ACCOMMODATION LADDER BOTTOM PLATFORM STANCHION SECURIING ARRANGEMENT OBSERVED TO BE SLAIGHTLY SHEARED.","Deck - Machinery","General Appearance","Equipment Related","5.47","Low","","","PLATFORM TO BE DISMANTLED AND TAKEN TO ER WORKSHOP FOR REPAIR AND THEN FIXED BACK.","2019-11-04","","Completed","2019-11-03","No","No","No","Internal"]
[null,null,null,null,7424,"52_15/11/2019 15:40:45","2019-11-04","Defect","Ship Staff","Ship Staff Insp.","Emergency fire Pump Mechanical Seal leaking","Critical Equip.,LSA / FFA","Safety / LSA / FFA","Equipment Related","10.29","Medium","","","Pump overhauled, Mechanical Seal Replaced","2019-11-30","","Completed","2019-11-07","No","No","No","Internal"]
[null,null,null,null,7415,"52_15-11-2019 15:07:28","2019-11-04","Defect","Ship Staff","Ship Staff Insp.","SAVE ALL TRAY FOR ONE MOORING WINCH ON POOP DECK OBSERVED TO BE WASTED AT 2 LOCATIONS.","Deck - Pipe / Fittings","Mooring","Equipment Related","6.9","Low","","","TEMPORARY REPAIRS HAVE BEEN MADE BY COLD WORK. VESSEL HAS TO BE GAS FREE TO CARRY OUT HOTWORK. JOB CREATED IN REFMAN","2020-10-31","","Completed","2020-04-01","Yes","No","No","Internal","Raise the same in REFMAN for the job to be carried out in DD."]
[null,null,null,null,7426,"52_15/11/2019 15:52:59","2019-11-09","Defect","Ship Staff","Ship Staff Insp.","Economiser water circulating line valve bonnet gasket leaking.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Valve Bonnet gasket replaced.","2019-11-10","","Completed","2019-11-09","No","No","No","Internal"]
[null,null,null,null,7416,"52_15-11-2019 15:13:56","2019-11-10","Defect","Ship Staff","Ship Staff Insp.","STBD WINDLASS OPERATING LEVER BLOCK  OBSERVED TO BE LEAKING. ","Deck - Machinery","Mooring","Equipment Related","9.14","Medium","","","leakage rectified by replacing o ring.","2019-11-30","EBAY190103","Completed","2020-02-05","No","No","No","Internal","Noted"]
[null,null,null,null,7428,"52_Sun Dec 01 2019 17:45:57 GMT+0000 (Coordinated Universal Time)","2019-11-11","Defect","Ship Staff","Ship Staff Insp.","Rescue boat davit falls hard plastic sheaves retaining wall has worn out. ","LSA / FFA","Safety / LSA / FFA","Equipment Related,Human Error,Inappropriate Procedure","5.28","Very High","","","All the sheaves have been inspected and 4 sheaves have been renewed.","2019-11-11","","Completed","2019-11-12","No","No","No","Internal"]
[null,null,null,null,7429,"52_Sun Dec 01 2019 17:53:44 GMT+0000 (Coordinated Universal Time)","2019-11-11","Defect","Ship Staff","Ship Staff Insp.","Port and stbd side accommodation ladder air filter/lubricators are corroded and broken.","Deck - Machinery","ISM Related","Equipment Related","5.47","Low","","","Air filter/lubricator for both port and stbd accommodation ladders have been renewed.","2019-11-21","","Completed","2019-11-14","No","No","No","Internal"]
[null,null,null,null,7418,"52_15/11/2019 16:03:38","2019-11-11","Defect","Ship Staff","Ship Staff Insp.","Flashback arrestor for Acytelene is more than 5 year old.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","5.26","Medium","","","renewed with new flashback arrestor and pr regulator","2019-12-30","EBAY190164","Completed","2020-02-20","No","No","No","Internal","Noted. Will be supplied soon."]
[null,null,null,null,7419,"52_15/11/2019 16:14:09","2019-11-11","Defect","Ship Staff","Ship Staff Insp.","6 Monthly Lub oil Analysis is due since 1st Sep 2019","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.7","Medium","","","Lub Oil sample Kit not available onboard","2019-12-30","EBAY195084","Completed","2019-12-20","No","No","No","Internal"]
[null,null,null,null,7427,"52_15/11/2019 16:25:50","2019-11-12","Defect","Ship Staff","Ship Staff Insp.","PV valve of 4(P) and 6(P) leaking.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.41","Very High","","","Valve lapping carried out and leaks rectified.","2019-11-30","","Completed","2019-11-24","No","No","No","Internal"]
[null,null,null,null,9741,"52_15/1/2020 2:10:43 AM","2019-11-16","Non Conformity","Ship Staff","Ship Staff Insp.","During senior officer inspection rounds, out 15 visitor IDs 5 were found to be missing are follow (ID No. 3, 6, 8, 10 & 12)","Miscellaneous","ISPS Related","Behaviour Based,Industry Issue,Knowledge Based","7.12","High","","","id cards replaced with new ones","2020-02-16","","Completed","2020-02-17","No","No","No","Internal","Noted"]
[null,null,null,null,7420,"52_Sat Jan 12 2019 19:52:34 GMT+0000 (Coordinated Universal Time)","2019-11-16","Defect","Ship Staff","Ship Staff Insp.","Limit switch (hook stop) for rescue boat davit is broken.","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.28","Very High","","","Limit switch renewed by ETO","2019-12-31","EBAY195095","Completed","2019-12-12","No","No","No","Internal"]
[null,null,null,null,7430,"52_Sat Jan 12 2019 18:01:38 GMT+0000 (Coordinated Universal Time)","2019-11-17","Defect","Ship Staff","Ship Staff Insp.","Aft ETA air motor filter/lubricator covers have corroded. The cover box is wasted due to corrosion.","Deck - Mooring Machinery","Mooring","Equipment Related","9.28","Medium","","","Air filter/lubricator cleaned, derusted and painted. New cover box fabricated and fixed.","2019-11-24","","Completed","2019-11-23","No","No","No","Internal"]
[null,null,null,null,7435,"52_Tue Feb 12 2019 11:00:13 GMT+0000 (Coordinated Universal Time)","2019-11-17","Defect","Ship Staff","Ship Staff Insp.","Aux. Boiler atomising valve flange gasket broken, leading to steam leak.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Gasket replaced.","2019-11-20","","Completed","2019-12-17","No","No","No","Internal"]
[null,null,null,null,7434,"52_Tue Feb 12 2019 09:57:33 GMT+0000 (Coordinated Universal Time)","2019-11-20","Defect","Ship Staff","Ship Staff Insp.","AE#1 JCW temperature was not maintaining.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","JCW thermostatic valve replaced with new spare.","2019-12-15","","Completed","2019-11-28","No","No","No","Internal"]
[null,null,null,null,7431,"52_Sat Jan 12 2019 18:05:50 GMT+0000 (Coordinated Universal Time)","2019-11-23","Defect","Ship Staff","Ship Staff Insp.","Safety hand rail on the bulwark on forecastle deck was bent.","Miscellaneous","General Appearance","Inappropriate Procedure","11.1","High","","","The hand rail has been straightened, derusted and painted.","2019-11-30","","Completed","2019-11-30","No","No","No","Internal"]
[null,null,null,null,9315,"52_23/12/2019 6:08:55 PM","2019-11-23","Non Conformity","Ship Staff","Ship Staff Insp.","While attempting to lower the freefall lifeboat by davit, it was observed that the launching release bar was not retracting completely by the main hydro pump for boat launching. Upon investigation it was found that the oil reservior for the hydro pump had very less oil and hence was ineffective in retracting the release bar completely. The resorvior was filled with oil and hydro pump was operated successfully to retract the launching release bar completely.","LSA / FFA","Safety / LSA / FFA","Behaviour Based,Equipment Related,Industry Issue,Knowledge Based","5.29","High","","","The reservoir tank for the hydro pump was filled to the correct level and the launching system was tested to check that the launching release bar is retracted completely by both the main hydro pump and emergency hydro pump. Senior officers should ensure during the simulation test that the launching release bar completely retracts by the hydro pump. Maintenance carried out by Junior Officers should be cross checked. Highligheted during safety meeting. ","2019-12-31","","Completed","2019-11-30","No","No","No","Internal"]
[null,null,null,null,7421,"52_Sat Jan 12 2019 19:56:13 GMT+0000 (Coordinated Universal Time)","2019-12-01","Defect","Ship Staff","Ship Staff Insp.","Midship crane hook assembly shackles are rusted and not free to open.","Deck - Machinery","Cargo / Ballast Systems","Equipment Related","8.5","Medium","","","De-rusted, made free, greased and lubricated and painted.","2019-12-08","","Completed","2019-12-12","No","No","No","Internal"]
[null,null,null,null,7432,"52_Sun Dec 01 2019 18:33:11 GMT+0000 (Coordinated Universal Time)","2019-12-09","Defect","Ship Staff","Ship Staff Insp.","Port ballast pump air ejector drive airline section wasted and holed due to corrosion.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.15","Medium","","","New pipe fabricated and replaced.","2019-12-16","","Completed","2019-12-12","No","No","No","Internal"]
[null,null,null,null,9319,"52_17/12/2019 2:21:36 PM","2019-12-12","Defect","Ship Staff","Ship Staff Insp.","Port side accommodation ladder railing cracked.","Miscellaneous","ISM Related","Equipment Related","5.47","Low","","","FABRICATION CARRIED OUT","2020-10-31","","Completed","2020-03-29","Yes","No","No","Internal","MAKE ALTERNATIVE RAILING OF DIFFERENT MATERIAL (MS PIPE).  ALUMINIUM RAILING CAN BE SUPPLIED LATER."]
[null,null,null,null,9321,"52_25-12-2019 18:45:41","2019-12-16","Other","Ship Staff","Ship Staff Insp.","AIR CONDITION NO.1 CONTROLLER MALFUNCTIONING","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","CONTROLLER TRPLACED WITH NEW SPARES ","2020-04-30","EBAY 190207","Completed","2020-03-20","No","No","No","Internal","PRE-PROGRAMMED AC CONTROLLER ORDERED EBAY205001 AND CONNECTED ON BOARD  @ ROTTERDAM ON 09TH MARCH 2020. VESSEL STAFF TO RENEW IT AND COMPLETE THE JOB."]
[null,null,null,null,9317,"52_25-12-2019 18:54:17","2019-12-19","Breakdown","Ship Staff","Ship Staff Insp.","Provision crane supply MCB not working and hydraulic hose leaky","Deck - Machinery","Eng. / Strg. Comp.","Equipment Related","8.5","Medium","","","Change the MCB and Hydraulic hose","2019-12-31","","Completed","2019-12-19","No","No","No","Internal"]
[null,null,null,null,9318,"52_25-12-2019 18:57:52","2019-12-22","Breakdown","Ship Staff","Ship Staff Insp.","Main Air Compressor No.1 unloader malfunctioning","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Change the unloader and try out","2019-12-29","","Completed","2019-12-22","No","No","No","Internal"]
[null,null,null,null,9322,"52_25-12-2019 19:08:35","2019-12-24","Critical Equipment","Ship Staff","Ship Staff Insp.","Waste oil incinerator solenoid  malfunctioning","Critical Equip.","MARPOL Related","Equipment Related","6.16","Very High","","","CHANGED WITH NEW SPARE","2019-12-31","EBAY200003","Completed","2020-03-16","No","No","No","Internal","When is the vessel raising a RO."]
[null,null,null,null,9745,"52_15/1/2020 2:22:36 AM","2019-12-25","Non Conformity","Ship Staff","Ship Staff Insp.","During pre-arrival tests/checks it was observed that the IGG main burner pump pressure gauge was defective, showing erratic reading and leaking.","Inert Gas","Cargo / Ballast Systems","Equipment Related,Industry Issue","8.25","Medium","","","The defective pressure gauge has been temporary replaced with higher range of gauge and requisition has been raised for the appropriate gauge as per maker. Discussed during safety meeting to keep sufficient spare pressure gauges on board and records of change to be maintained in PMS. ","2020-01-25","","Completed","2019-12-30","No","No","No","Internal"]
[null,null,null,null,9742,"52_07/01/2020 11:51:38 AM","2019-12-29","Defect","Ship Staff","Ship Staff Insp.","Midship hose handling crane pressure gauge was observed not functioning.","Deck - Machinery","Cargo / Ballast Systems","Equipment Related","8.5","Medium","","","Renewed with spare pressure gauge","2020-01-02","","Completed","2019-12-30","No","No","No","Internal"]
[null,null,null,null,10786,"52_11/2/2020 2:06:43 PM","2020-01-12","Defect","Ship Staff","Ship Staff Insp.","Aux.Engine fuel filter block leaking","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","CHANGED WITH NEW BLOCK","2020-03-12","EBAY200010","Completed","2020-03-15","No","No","No","Internal"]
[null,null,null,null,10781,"52_11/2/2020 2:23:35 PM","2020-01-14","Defect","Ship Staff","Ship Staff Insp.","Aux. boiler flowmeter faulty","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Cleaned line filter and flowmeter inlet filter.changed flow through bypass// RENEWED THE FLOW METER WITH NEW FLOWMETER RECIEVED AT BOSTON ","2020-05-30","EBAY200042","Completed","2020-05-29","No","No","No","Internal","EBAY200042 AUX BOILER FO FLOW METER ORDERED. SPARES CONNECTED ON BOARD. ONCE RENEWED, CLOSE THE OBSERVATION."]
[null,null,null,null,10782,"52_11/2/2020 2:37:44 PM","2020-01-15","Defect","Ship Staff","Ship Staff Insp.","IGG Capacity control valve actuater malfunctioning.","Inert Gas","Cargo / Ballast Systems","Equipment Related","8.25","Medium","","","REPLACED THE ACTUATOR AND POSITIONOR. THE VALVE WAS ALSO DISMANTLED AND CLEANED FOR SMOOTH OPERATION ","2020-04-15","EBAY200038","Completed","2020-03-15","Yes","No","No","Internal","IGG Capacity Valve spares was ordered under requisition EBAY200038 and connected at Rotterdam @10 March 2020. Please carry out repairs with spares supplied and revert!"]
[null,null,null,null,10787,"52_11/2/2020 2:43:12 PM","2020-01-18","Defect","Ship Staff","Ship Staff Insp.","Aux.Engine #3 jacket cooling  thermostatic walve malfunction","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","CHANGED WITH NEW SPARE","2020-03-18","EBAY200010","Completed","2020-03-13","No","No","No","Internal"]
[null,null,null,null,10788,"52_27/2/2020 10:21:50 AM","2020-01-19","Defect","Ship Staff","Ship Staff Insp.","9 Framo Pressure Gauges inoperational and 2 snap on coupling broken","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.8","Very High","","","replaced with new pr gaues ","2020-04-19","EBAY200039","Completed","2020-02-16","No","No","No","Internal"]
[null,null,null,null,10789,"52_02/03/2020 5:06:09 AM","2020-02-14","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","SMPEP Locker Absorbent Pads and Booms detoriating and flaking","Critical Equip.","Emgcy. Systems","Equipment Related","6.3","Low","","","NEW ITEMS RECIEVED AND REPLACED. SMPEP EQUIPMENT LIST UPDATED AND POSTED IN THE LOCKER.","2020-02-20","","Completed","2020-02-18","No","No","No","Internal","NOTED."]
[null,null,null,null,10790,"52_02/03/2020 5:09:29 AM","2020-02-14","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Water leak from Deck seal SW Pump 2","Inert Gas","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","LEAK RECTIFIED, PACKING CHANGED","2020-03-26","","Completed","2020-02-20","No","No","No","Internal"]
[null,null,null,null,10791,"52_02/03/2020 5:25:47 AM","2020-02-14","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Gym equipments are kept in Air condition room instead of Gymnasium","Miscellaneous","MLC Related","Inappropriate Procedure","","","","","TRNSFERED TO GYMNASIUM","2020-05-14","","Completed","2020-02-17","No","No","No","Internal"]
[null,null,null,null,10792,"52_02/03/2020 5:30:27 AM","2020-02-14","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Manholes of WBT’s having rust and rust stains near the bolts area","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.3","Medium","","","CIHPPING AND PAINTING DONE ON SAME, ALL FOUND SATISFACTORY","2020-05-14","","Completed","2020-02-21","No","No","No","Internal"]
[null,null,null,null,10793,"52_02/03/2020 5:39:49 AM","2020-02-14","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Wilden pump for transferring contents of Drip tray to ROT not working","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.8","Very High","","","REQUISITION RAISED","2020-05-14","EBAY200050","Completed","2020-02-21","No","No","No","Internal"]
[null,null,null,null,10794,"52_02/03/2020 5:52:00 AM","2020-02-14","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Stbd windlass and Aft Spring winch Control lever unit leaking","Deck - Mooring Machinery","Mooring","Equipment Related","9.14","Medium","","","O RING REPLACED AND LEAK RECTIFIED","2020-05-14","","Completed","2020-02-21","No","No","No","Internal"]
[null,null,null,null,10795,"52_02/03/2020 5:56:11 AM","2020-02-14","Non Conformity","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Eyewash kept in Paint store is Half Empty","Miscellaneous","Safety / LSA / FFA","Inappropriate Procedure","5.46","Medium","","","REPLACED WITH NEW","2020-02-15","","Completed","2020-02-14","No","No","No","Internal"]
[null,null,null,null,10803,"52_03/03/2020 7:13:35 AM","2020-02-14","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Safety contour and Safety Depth values wrongly calculated in passage plan from Puerto Moin to Baton Rogue","Navigation - Others","Navigation","Knowledge Based","4.14","Very High","","","Discussed/highlighted to the person in-charged  the subject matter. Amendment of Passage Plan carried out as attached. Bridge team meeting carried out , master  briefed about the correct procedures for putting safety settings and gave instruction for double checking of passage plan after entering values.","2020-05-14","","Completed","2020-02-20","No","No","No","Internal"]
[null,null,null,null,17539,"52_Tue Jan 19 2021 05:31:10 GMT+0000","2020-02-14","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Wire mesh of Natural Vent no 32 of Bosun Store dislodged","Deck - Pipe / Fittings","General Appearance","External Factors","","","","","Vent Mesh is in good state. It was removed and refitted back.","2020-02-29","","Completed","2020-02-27","No","No","No","Internal","Noted."]
[null,null,null,null,17540,"52_Tue Jan 19 2021 05:53:54 GMT+0000","2020-02-14","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Windlass and Mooring winches having Rust patches","Deck - Mooring Machinery","General Appearance","External Factors","","","","","De-rusting and painting of windlass and Mooring winches completed.","2020-02-29","","Completed","2020-02-27","No","No","No","Internal","Noted."]
[null,null,null,null,17541,"52_Tue Jan 19 2021 06:01:09 GMT+0000","2020-02-14","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Razor wires kept in Bosun store to be covered and marked “CAUTION – RAZOR WIRES HAVING\nSHARP EDGES”","Miscellaneous","Safety / LSA / FFA","Behaviour Based","","","","","Razor wire covered and Markings done as required.",null,"","Completed","2020-02-16","No","No","No","Internal","Razor wire always must be covered and marked with Caution  - \"Razor wires having sharp edges.\""]
[null,null,null,null,17542,"52_Tue Jan 19 2021 06:04:58 GMT+0000","2020-02-14","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","No MSDS in place for Glycol kept in Paint store","Miscellaneous","Cert. & Docu.","Knowledge Based","","","","","MSDS for Glycol posted in paint store","2020-02-25","","Completed","2020-02-22","No","No","No","Internal","Noted."]
[null,null,null,null,17543,"52_Tue Jan 19 2021 06:13:19 GMT+0000","2020-02-14","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Cargo tank domes covers having rust patches.","Hull & Tanks","Cargo / Ballast Systems","External Factors","","","","","De-rusting and painting of tank domes in completed.","2020-02-29","","Completed","2020-02-27","No","No","No","Internal","Noted."]
[null,null,null,null,17544,"52_Tue Jan 19 2021 06:15:26 GMT+0000","2020-02-14","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Some U-Clamps of Deck pipelines in Poor condition.","Deck - Pipe / Fittings","General Appearance","External Factors","","","","","All U Clamps Derusted and Painted - Reconditioning of u clamps completed.","2020-02-29","","Completed","2020-02-27","No","No","No","Internal","Noted."]
[null,null,null,null,17545,"52_Tue Jan 19 2021 06:29:35 GMT+0000","2020-02-14","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","TO VERIFY HEATER FOR EMERGENCY SHOWER IS WORKING.","LSA / FFA","Emgcy. Systems","Equipment Related","","","","","Heater line operational.","2020-02-15","","Completed","2020-02-15","No","No","No","Internal","NOTED."]
[null,null,null,null,17546,"52_Tue Jan 19 2021 06:43:56 GMT+0000","2020-02-14","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","VDR ACOUSTIC BEACON BATTERY TO RENEW DURING ANNUAL SERVICE.","Navigation - VDR / BNWAS","Navigation","Equipment Related","","","","","BATTERY RENEWED DURING SERVICE.","2020-02-25","","Completed","2020-02-18","No","No","No","Internal","NOTED."]
[null,null,null,null,10796,"52_29/02/2020 07:25:04","2020-02-17","Critical Equipment,Defect","Ship Staff","Ship Staff Insp.","EMERGENCY FIRE PUMP MECHANICAL SEAL LEAKING","E/R - Pumps","Safety / LSA / FFA","Equipment Related","10.29","Medium","","","FIRE PUMP OVERHAULED . REPLACED MECHANICAL SEAL AND O RINGS. PUMP PARTS INSPECTED. PUMP BOXED BACK AND TRIED OUT AND FOUND TO BE SATISFACTORY.","2020-02-20","","Completed","2020-02-18","No","No","No","Internal"]
[null,null,null,null,10797,"52_29/2/2020 9:15:20 AM","2020-02-18","Defect","Ship Staff","Ship Staff Insp.","MAIN FIRE PUMP MECHANICAL SEAL LEAKING . LEAKAGES OBSERVED DURING THE SATURDAY ROUTINES TEST. ","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","PUMP DISMANTLED, ALL PARTS CLEANED AND INSPECTED. RENEWED MECHANICAL SEAL AND O RINGS. PUMP BOXED BACK AND TRIED OUT. FOUND TO BE SATISFACTORY. ","2020-02-20","","Completed","2020-02-20","No","No","No","Internal"]
[null,null,null,null,10784,"52_29/2/2020 9:18:54 AM","2020-02-22","Critical Equipment","Ship Staff","Ship Staff Insp.","EMERGENCYGENERATOR JACKET WATER HEATER FOUND TO HAVE LOW INSULATION AND NEED TO BE REPLACED","Critical Equip.","Emgcy. Systems","Equipment Related","10.38","Medium","","","REPLACED THE HEATER AND THE THERMOSTAT WITH NEW SPARE RECIEVED ONBOARD. SYSTEM TRIED OUT AND FOUND TO BE SATISAFACTORY.","2020-04-01","EBAY200108","Completed","2020-03-29","No","No","No","Internal","Ordered New Heater, Thermostat and Cable under Requisition EBAY200108. Once spares are ready, will be connected on board."]
[null,null,null,null,10798,"52_02/03/2020 6:46:56 AM","2020-02-24","Observation","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","There were no records that all cargo tanks were physically checked for pressure and oxygen level prior commencement of cargo operations. Physical checks were not carried out/recorded for pressure and oxygen level as required by SSSCL item 19 & 20 - repetitive checks.","Documentation","Cargo / Ballast Systems","Knowledge Based","5.9","Very High","","","STARTED MAINTING LOG IN CCR LOG BOOK AS WELL AS IN O2 LOG PRIOR ARRIVAL PORT , BRIEFING DONE TO ALL CREW BY MASTER","2020-02-25","","Completed","2020-02-25","No","No","No","External"]
[null,null,null,null,10799,"52_02/03/2020 6:54:43 AM","2020-02-24","Observation","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","Areas on the enclosed lifeboats where personnel may walk did not have an effective non-slip surfaces. Original non slip surfaces were painted over with numerous coats of paint over the years and diminishing its effectiveness.","Critical Equip.","Safety / LSA / FFA","Knowledge Based","5.29","High","","","Re-painted with more non-skid paint in the lifeboat walkway","2020-02-29","","Completed","2020-02-26","No","No","No","External"]
[null,null,null,null,11277,"52_03/04/2020 11:45:07 AM","2020-02-26","Non Conformity","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ENGINE ROOM AND BRIDGE MOVEMENT BOOK  ENTRIES NOT MADE AS PER THE GUIDANCE GIVEN IN THE MOVEMENT  BOOK, SOME REQUIRED ENTRY MISSING.","Documentation","ISM Related","Human Error,Knowledge Based","4.2","Medium","","","BRIEFING DONE AND STARTED MAKING ENTRIES AS PER REQUIREMENTS.","2020-02-29","","Completed","2020-02-28","No","No","No","Internal"]
[null,null,null,null,10785,"52_29/2/2020 9:25:04 AM","2020-02-26","Breakdown","Ship Staff","Ship Staff Insp.","GALLEY FOOD WASTE DISPOSER FOUND TO GIVE LOW INSULATION. ON INSPECTION FOUND THE SEAL DAMGED AND THE MOTOR WINDINGS SOAKED IN WATER .","Accommodation","MARPOL Related","Equipment Related","11.16","Low","","","EQUIPMENT ISOLATED AND MOTOR MOTOR OVERHAULED, RENEWED SEALS AND THE DAMAGED PARTS WITH NEW SPARES. INSTALLED THE MOTOR AFTER OVERHAULING. TRIED OUT AND FOUND TO BE SATISFACTORY. ","2020-05-10","EBAY200094- GALLEY WASTE DISPOSER","Completed","2020-03-30","No","No","No","Internal","Ordered EBAY200094 – GALLEY WASTE DISPOSER SPARES and will be connected to vessel at Port Everglades, USA on@24th March 2020."]
[null,null,null,null,10800,"52_29/2/2020 9:27:53 AM","2020-02-27","Defect","Ship Staff","Ship Staff Insp.","DECK AIR COMPRESSOR AIR HOSES FOUND TO HAVE LEAKAGES ","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","CHANGED WITH NEW HOSE","2020-05-15","EBAY200110","Completed","2020-03-16","No","No","No","Internal"]
[null,null,null,null,10801,"52_16/3/2020 4:33:56 AM","2020-03-01","Defect","Ship Staff","Ship Staff Insp.","HFO PURIFIER FEED PUMP NO.1 SEAL LEAKING","E/R - Purifier","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","RENEWED SEASL WITH NEW SPARE","2020-03-30","","Completed","2020-03-13","No","No","No","Internal"]
[null,null,null,null,10783,"52_3/3/2020 11:17:01 AM","2020-03-11","Defect","Ship Staff","Ship Staff Insp.","DECK EYE WASH SYSTEM LINE INSULATION AT FEW LOCATIONS TO IMPROVISE.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","HEATER IS WORKING. SOME PLACES INSULATION IS BEING IMPROVISED.","2020-05-31","EBAY20074 / EBAY200102","Completed","2020-05-15","No","No","No","Internal","NOTED WORK CARRIED OUT. ALWAYS OPERATE HEATER INBETWEEN TO VERIFY IT'S OPERATION."]
[null,null,null,null,10802,"52_16/3/2020 4:30:31 AM","2020-03-14","Critical Equipment","Ship Staff","Ship Staff Insp.","ODME SAMPLE PUMP JAMMED","Critical Equip.","MARPOL Related","Equipment Related","6.13","Low","","","CRITICAL WORK PERMIT OBTAINED JOB CARRIED OUT FOUND WORKING SATISFACTORY","2020-03-30","","Completed","2020-03-16","No","No","No","Internal"]
[null,null,null,null,11278,"52_30/3/2020 2:15:17 PM","2020-03-26","Defect","Ship Staff","Ship Staff Insp.","WASTE OIL INCINERATOR  COMBUSTION CHAMBER TEMPERATURE SENSOR WAS FOUND TO BE DEFECTIVE ","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","6.16","Very High","","","REPLACED THE TEMPERATURE SENSOR WITH THE SPARE SENSOR FROM CRITICAL SPARES. NEW REQUISITION FOR THE USED SPARE RAISED FROM VESSEL FOR REPLACEMENT IN  CRITICAL SPARES","2020-03-28","EBAY200124","Completed","2020-03-26","No","No","No","Internal"]
[null,null,null,null,7433,"52_Sun Dec 01 2019 18:38:38 GMT+0000 (Coordinated Universal Time)","2020-03-31","Defect","Ship Staff","Ship Staff Insp.","Mechanical vent heads on bridge deck mesh retaining rings wasted.","Deck - Machinery","General Appearance","Equipment Related","11.7","High","","","new ring fabricated and installed","2020-06-30","EBAY200127","Completed","2020-05-24","Yes","No","No","Internal","AS SUGGESTED IN EMAIL, PLEASE REMOVE ALL SUBJECT VENTS ONE BY ONE, BRING TO WORKSHOP, CARRY OUT REPAIRS, PAINT THEM AND FIX BACK."]
[null,null,null,null,12034,"52_30/05/2020 12:44:06 PM","2020-04-15","Defect","Ship Staff","Ship Staff Insp.","E/R BLOWERS ON FUNNEL DECK SUPPORT BROKEN AND ELECTRICAL JUNCTION BOX FOUND TO HAVE HOLES","Accommodation,Deck - Pipe / Fittings,Elect. Mach. & Equip.","Structural Condn. / WT integrity ","Equipment Related","11.3","Medium","","","Temporary repairs carried out, terminal box to be removed and repaired.","2020-09-30","","Completed","2020-06-30","No","No","No","Internal","JUNCTION BOX REMOVED, FABRICATED AND FITTED .  REPAIRS ARE COMPLETED FULLY."]
[null,null,null,null,12035,"52_31/5/2020 12:21:59 PM","2020-04-15","Defect","Ship Staff","Ship Staff Insp.","INCINERATOR REFRACTORY IS DAMAGED AT  DIFFERENT LOCATION AND NEEDS COMPLETE REPALCEMENT WITH WORKSHOP ASSISTANCE","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","INFORMED OFFICE AND ADDED TO REFMAN FOR FUTHER REFERENCE","2020-07-15","","Completed","2020-06-30","No","No","No","Internal","REFRACTORY REPAIRS CARRIED OUT BY STAFF ARE  HOLDING OK AT THE PRESENT AND WE WILL MONITOR SITUATION GOING FORWARD."]
[null,null,null,null,12036,"52_30/05/2020 12:48:33 PM","2020-04-24","Defect","Ship Staff","Ship Staff Insp.","PAINT STORE AND SMPEP GEAR LOCKER MECHANICAL VENTS HAVE THINNED DOWN AND HAVE SOFT PATCHES TO COVER HOLE","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","External Factors","11.4","Very High","","","Soft patch applied and touchup done. fabrication in progress \n\nRENEWED DAMGED PORTION OF THE MECHANICAL VENT HEADS AND REPAIRSD DONE. PAINTED AND INSTALLED IN PLACE ","2020-09-30","","Completed","2020-07-04","No","No","No","Internal"]
[null,null,null,null,12038,"52_31/5/2020 12:25:42 PM","2020-05-22","Breakdown","Ship Staff","Ship Staff Insp.","NO 1 HFO PURIFIER MOTOR WINDINGS DAMAGED AND NEED REPLACEMENT OF MOTOR","E/R - Purifier","Eng. / Strg. Comp.","Equipment Related","","","","","REQUISITION RAISED FOR MOTOR AWAITING SUPPLY\n\nREPLACED THE DAMGED MOTOR WITH A NEW SPARE MOTOR. PURIFIER TRIED OUT AND FOUND TO BE SATISFACTORY. ","2020-07-31","EBAY200139","Completed","2020-07-15","No","No","No","Internal","NEW MOTOR WILL BE CONNECTED AT PORT JEROME. ONCE RECEIVED, REPLACE IT."]
[null,null,null,null,12040,"52_31/5/2020 12:42:35 PM","2020-05-23","Defect","Ship Staff","Ship Staff Insp.","SEA WATER PIPE FOUND TO HAVE LEAKAGES ","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","PIPE REPAIRED AND TESTED . FOUND TO HAVE NO LEAKAGES . ","2020-05-25","","Completed","2020-05-24","No","No","No","Internal"]
[null,null,null,null,12041,"52_02/06/2020 8:00:51 AM","2020-05-28","Observation","PSC Insp.","PSC Inspection","EACH LIFERAFT SHALL BE STOWED WITH FLOAT FREE ARRANGEMENT, THE PORT SIDE LIFERAFT PAINTER WAS NOT CONNECTED TO THE WEAK LINK.","LSA / FFA","Safety / LSA / FFA","Human Error","5.28","Very High","Life saving appliances","","Painter was immediately secured to the correct position in front of the inspector.Master briefed all officer’s and crew on the correct procedures for securing and use of liferafts, training session and safety video shown to all staff. Responsible person instructed to check securing arrangement at regular intervals ","2020-05-30","","Completed","2020-05-28","No","No","No","External"]
[null,null,null,null,12039,"52_31/5/2020 1:03:49 PM","2020-05-29","Breakdown","Ship Staff","Ship Staff Insp.","FORWARD ELECTRIC HORN , HORN PIPE ( FRP MATERIAL) FOUND TO BE CRACKED . NEED TO REPLACE THE HORN PIPE","Navigation - Others","Navigation","Equipment Related","11.4","Very High","","","REMPORARY REPAIRS DONE AND PAINTED. NEED TO REPLACE THE HORN PIPE// REPLACED THE HORN PIPE WITH NEW SPARE , TRIED OUT HORN AND FOUND TO BE OPERATIONAL","2020-07-30","EBAY200141","Completed","2020-07-16","No","No","No","Internal","We reviewed repairs carried out, found OK. Please arise requisition for horn only. It usually have long delivery time. Till that period keep monitoring to avoid complete breaking of horn in two pieces."]
[null,null,null,null,12037,"52_30/05/2020 12:52:31 PM","2020-06-09","Defect","Ship Staff","Ship Staff Insp.","ME FUNNEL PIPE THINNED DOWN AND CRACK FROM BOTH SIDE.","E/R - Pipes/ valves & fittings","Structural Condn. / WT integrity ","Equipment Related","10.38","Medium","","","derusted and painted, fabrication to be done. THE FUNNEL PIPE WAS SECURED FROM ALL SIDES USING BOTTLE SCREWS AND WIRES. CEMENT BOX FABRICATED BELOW THE PIPE TO COVER THE CRACK . TEMPORARY REPAIRS DONE TO COVER UP THE DAMAGED PORTION OF THE PIPE.","2020-09-30","","Completed","2020-08-15","No","No","No","Internal","REPAIRS CARRIED OUT ARE  HOLDING GOOD."]
[null,null,null,null,4904,"52_25/10/2019 9:29:41 AM","2020-06-25","Defect","Ship Staff","Ship Staff Insp.","PORT AND STBD SIDE ANCHOR CHAIN COMMON AND ENLARGED LINK STUDS THICKNESS HAS REDUCED AND MISSING, NEED TO BE RENEWED.","Deck - Machinery","Mooring","Equipment Related","9.2","Very High","","","REQUISITION RAISED. VESSEL HAS TO BE GAS FREE FOR HOTWORK TO BE CARRIED OUT.// RECVD SPARE CHAIN LINK STUDS ONBOARD / WILL REPALCE THEM AT SUITABLE OPPERTUNITY. // STUDS REPLACED WITH SPARE ONES// ","2020-08-31","EBAY190198","Completed","2020-08-28","No","No","No","Internal","STUDS ORDER IS PLACED AND WILL BE CONNECTED ON BOARD AT PORT JEROME.  ONCE RECEIVED, HAVE THEM WELDED AT RIGHT OPPORTUNITY."]
[null,null,null,null,13327,"52_14/7/2020 10:50:05 AM","2020-07-01","Breakdown","Ship Staff","Ship Staff Insp.","AUX ENGINE NO 2 THERMOSTATIC VALVE FOR COOLING WATER NOT OPERATIONAL.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","NEED TO REPALCE THE THERMOSTATIC VALVE / REQUISITION RAISED/ SUPPIED SPARES ONBOARD/ REPLACED THERMOSTATIC VALVE WITH NEW SPARE AND FOUND TO BE OPERATIONAL ","2020-07-30","EBAY200077","Completed","2020-07-16","No","No","No","Internal"]
[null,null,null,null,13328,"52_14/7/2020 10:44:44 AM","2020-07-09","Breakdown","Ship Staff","Ship Staff Insp.","SEWAGE TREATMENT PLANT DISCHARGE PUMP WAS FOUND TO BE DAMAGED. FEW PARTS INSIDE WAS FOUND TO BE CORRODED AND REQUIRE REPLACEMENT. ","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","NEW REQUISITION WAS RAISED FOR THE SPARES AND SUPPLIED ON BOARD. REPLACED THE DAMAGED PUMP WITH NEW SPARE PUMP AND MOTOR AND TRIED OUT. WORKING SATISFACTORLLY. ","2020-07-15","EBAY200030","Completed","2020-07-14","No","No","No","Internal"]
[null,null,null,null,13323,"52_31/07/2020 6:57:12 PM","2020-07-16","Observation","Ship Staff","Ship Staff Insp.","IMO symbols have faded in many locations","LSA / FFA","Safety / LSA / FFA","External Factors","5.31","High","","","Need to be replaced, requisition raised.// IMO SYMBOLS RENEWED ","2020-08-15","EBAY200162","Completed","2020-08-20","No","No","No","Internal"]
[null,null,null,null,13324,"52_31/07/2020 7:02:24 PM","2020-07-16","Observation","Ship Staff","Ship Staff Insp.","Eye wash expired. Face shield and chemical goggles not available.","Miscellaneous","Safety / LSA / FFA","Human Error","5.46","Medium","","","Requisition raised// RECVD STORES AND REPLENISED THE EYE WASH AND FACE SHIELDS ","2020-08-16","EBAY200162","Completed","2020-08-18","No","No","No","Internal"]
[null,null,null,null,13326,"52_31/07/2020 7:14:38 PM","2020-07-16","Observation","Ship Staff","Ship Staff Insp.","Stbd ballast pump gauge glass broken.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.8","Very High","","","Gauge renewed upon receipt","2020-09-16","EBAY200165","Completed","2020-09-12","No","No","No","Internal","SPARES ARE ORDERED, DISPATCHED AND WILL BE CONNECTED TO VESSEL SHORTLY."]
[null,null,null,null,13329,"52_31/07/2020 7:17:34 PM","2020-07-16","Observation","Ship Staff","Ship Staff Insp.","Fresh water and air line isolation valve wheels wasted and broken\t","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.4","Very High","","","To be renewed  / Renewed with spare valve wheels","2020-07-20","","Completed","2020-07-18","No","No","No","Internal"]
[null,null,null,null,17483,"52_Mon Jan 18 2021 06:24:07 GMT+0000","2020-07-16","Observation","Owner / Marine / Tech. Suptd.","Mooring Audit","REMOTE MOORING AUDIT:-Six numbers of Mooring ropes were found with more than SDMBL. SDMBL of the vessel is 51t and the six ropes had LDBF of 59-63 t.","Deck - Mooring Machinery","Mooring","Equipment Related","9.5","High","","","The vessel was supplied with Mooring ropes of correct LDBF.","2020-10-16","","Completed","2020-08-07","No","No","No","Internal","All mooring ropes are in compliance with LDBF as required by the vessel."]
[null,null,null,null,17484,"52_Mon Jan 18 2021 06:28:15 GMT+0000","2020-07-16","Observation","Owner / Marine / Tech. Suptd.","Cargo Audit","Remote Cargo Audit:-=The Cargo plan did not include the information provided by the charterers","Miscellaneous","ISM Related","Inappropriate Procedure","8.5","Medium","","","The vessel has included the voyage order in the Cargo Plan going forward.","2020-10-16","","Completed","2020-07-25","No","No","No","Internal","Verified"]
[null,null,null,null,14198,"52_06/10/2020 2:34:17 PM","2020-07-16","Observation","Ship Staff","Ship Staff Insp.","Lifeboat sighting ports observed to be very hazy.","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.26","Medium","","","All lifeboat sighting ports renewed.","2020-09-30","","Completed","2020-09-21","No","No","No","Internal"]
[null,null,null,null,13330,"52_03-08-2020 12:36:10","2020-07-25","Observation","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","Vessel has 16 HMPE lines on drums. 10 have MBL of 51 tons, 2 have MBL of 59.6 and 4 have MBL of 62.4. Ship design MBL is 51 tonnes. Lines are all same diameter and length. Brakes set to render at 25.5 T","Deck - Mooring Machinery","Mooring","Inappropriate Procedure","9.5","High","","","Mooring ropes with the LDBF as per MEG4, i.e. LDBF 100~105% higher than ship design MBL, will be supplied to the vessel as and when the ropes are renewed (by the inspection criteria as per company procedures). The mooring ropes with higher similar MBL have been transferred to aft mooring winches. Additionally, it may also be noted that the brakes on all mooring winches have been set to render at 60% of the Ship Design MBL which was mistakenly set to render at 50% of the design MBL that was 25.5T. ","2020-08-25","","Completed","2020-07-28","No","No","No","External"]
[null,null,null,null,13734,"52_31-08-2020 13:54:15","2020-08-12","Observation","Ship Staff","Ship Staff Insp.","Sampling tubes behind VECS panel detiriorated.","Inert Gas","Cargo / Ballast Systems","Equipment Related","8.17","Medium","","","Sampling tubes renewed.","2020-08-15","","Completed","2020-08-13","No","No","No","Internal"]
[null,null,null,null,13729,"52_22/8/2020 9:31:32 PM","2020-08-17","Breakdown","Ship Staff","Ship Staff Insp.","HOSE HANDLING CRANE HOISTING MOTOR HYDRAULIC BLOCK WAS FOUND TO BE DAMAGED . THE COUNTERBALANCE VALVE IS LEAKING.","Deck - Machinery","Cargo / Ballast Systems","Equipment Related","","","","","RECEIVED  NEW HOISTING BLOCK, REPLACED OLD ONE TRIED OUT WORKING SATISFACTORY","2020-09-15","EBAY205055 RECIVED ON 10th SEP 2020","Completed","2020-09-29","No","No","No","Internal","EBAY205055 ORDERED, DISPATCHED AND ALREADY WITH LOCAL AGENT/BAYTOWN, USA. IT WILL BE CONNECTED TO VESSEL ONCE ALONGSIDE."]
[null,null,null,null,13735,"52_22/8/2020 9:34:56 PM","2020-08-20","Defect","Ship Staff","Ship Staff Insp.","DECK SEAL PUMP DISCHERGE SIDE SACRIFICIAL FLANGE WAS FOUND TO BE LEAKING AND REQUIRE TO BE RENEWED. ","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","RENEWED THE FLANGE AND LEAKAGES RECTIFIED.","2020-08-22","","Completed","2020-08-22","No","No","No","Internal"]
[null,null,null,null,13728,"52_31-08-2020 13:57:50","2020-08-25","Defect","Ship Staff","Ship Staff Insp.","2 UTI showing \"No message\" alarm when switched on.","Miscellaneous","Cargo / Ballast Systems","Equipment Related","8.22","Very High","","","Shore servicing / calibration carried out.","2020-09-30","EBAY200186","Completed","2020-09-10","No","No","No","Internal","AS PER FEEDBACK, 1 UTI OUT OF  2 IS MADE FUNCTIONAL. ALSO SERVICE ARRANGEMENT CONFIRMED FOR ATTENDING AT UPCOMING PORT BAYTOWN."]
[null,null,null,null,13731,"52_29/8/2020 11:01:50 AM","2020-08-25","Defect","Ship Staff","Ship Staff Insp.","INERT GAS SYSTEM DECK LINE PRESSURE SENSOR FOUND TO BE DEFECTIVE . NEED TO REPLACE THE SENSOR .","Inert Gas","Cargo / Ballast Systems","Equipment Related","","","","","THE NEW SENSOR FITTED ON IG MAIN LINE. WORKING SATISFACTORY","2020-09-25","EBAY200183 RECIVED ON 10th SEP 2020","Completed","2020-09-12","No","No","No","Internal","ALREADY SHIP STAFF HAS PLACED ALTERNATIVE SPARE FOR MEASURING IG PRESSURE.                                            \n EBAY200183 ORDERED AND DISPATCHED TO CONNECT TO VESSEL AT UPCOMING PORT BAYTOWN, USA."]
[null,null,null,null,13732,"52_29/8/2020 11:05:43 AM","2020-08-25","Defect","Ship Staff","Ship Staff Insp.","ONE OF THE THERMOSTATIC EXPANSION VALVES FOR NO 1 EVAPORATOR FOR ACCOMODATION AC FOUND TO BE MALFUNCTIONING","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","NEW THERMOSTATIC EXPANSION VALVE REPLACED KEPT IN SERVICE, WORKING SATISFACTORY.","2020-09-21","EBAY200182, RECIVED ON 10th SEP 2020","Completed","2020-09-14","No","No","No","Internal","EBAY 200182 ORDERED ALREADY AND WILL BE CONNECTED TO VESSEL AT UPCOMING PORT BAYTOWN, USA."]
[null,null,null,null,13733,"52_31-08-2020 14:02:54","2020-08-27","Defect","Ship Staff","Ship Staff Insp.","2 multigas detectors not switching on.","Miscellaneous","Cargo / Ballast Systems","Equipment Related","5.23","Very High","","","Defective gas detectors replaced with refurbished ones.","2020-09-15","","Completed","2020-09-10","No","No","No","Internal","NEW DETECTORS ORDERED FOR REPLACEMENT AND ALREADY DISPATCHED TO CONNECT TO VESSEL."]
[null,null,null,null,15111,"52_Tue Nov 24 2020 05:26:54 GMT+0000","2020-09-07","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Cable and hydraulic lines supporting tray under the catwalk is corroded and wasted in some places, same to be renewed.","Deck - Pipe / Fittings","General Appearance","Equipment Related","","","","","Vessel has fabricated majority of the bad trays. Requisition has been raised for flat bars to renew the remaining.","2020-12-31","","Completed","2020-12-31","No","No","No","Internal","VESSEL TO RENEW ALL WASTED TRAYS AND COAT THEM."]
[null,null,null,null,15112,"52_Tue Nov 24 2020 05:30:09 GMT+0000","2020-09-07","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Bridge wing MOB marker ropes faded, to be renewed.","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","FADED ROPES TO RENEW WITH SPARE ONES.","2020-09-15","","Completed","2020-09-15","No","No","No","Internal","NOTED."]
[null,null,null,null,15113,"52_Tue Nov 24 2020 05:33:24 GMT+0000","2020-09-07","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Battery room door packing to be renewed.","Deck - Machinery","Structural Condn. / WT integrity ","Inappropriate Procedure","","","","","RENEW PACKING.","2020-09-15","","Completed","2020-09-15","No","No","No","Internal","PACKING RENEWED."]
[null,null,null,null,15114,"52_Tue Nov 24 2020 05:35:59 GMT+0000","2020-09-07","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Shore gangway ropes faded and wearing out, to be renewed.","Deck - Machinery","Safety / LSA / FFA","Inappropriate Procedure","","","","","FADED ROPE TO RENEW.","2020-09-15","","Completed","2020-09-15","No","No","No","Internal","SUBJECT ROPE RENEWED."]
[null,null,null,null,15115,"52_Tue Nov 24 2020 05:38:57 GMT+0000","2020-09-07","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","One deck stand roller found hard to turn, to be made free. Vessel to strictly follow the greasing schedule.","Deck - Machinery","Mooring","Inappropriate Procedure","","","","","TO FREE UP ROLLER AND GREASE. FOLLOW GREASING ROUTINE REGULARLY TO PREVENT ANY SEIZURE.","2020-09-15","","Completed","2020-09-15","No","No","No","Internal","GREASING ROUTINE MUST BE FOLLOWED STRICTLY AND REGULARLY."]
[null,null,null,null,15116,"52_Tue Nov 24 2020 05:41:35 GMT+0000","2020-09-07","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Void space manholes stencil of enclosed space not made after maintenance work. Stencil to be put.","Miscellaneous","General Appearance","Inappropriate Procedure","","","","","STENCILING DONE.","2020-09-15","","Completed","2020-09-15","No","No","No","Internal","NOTED."]
[null,null,null,null,15117,"52_Tue Nov 24 2020 05:45:12 GMT+0000","2020-09-07","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Vapour manifold bolts short in length, requisition raised for same. To be renewed once received.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Inappropriate Procedure","","","","","TO RENEW WITH APPROPRIATE LONG BOLTS.","2020-11-15","","Completed","2020-10-31","No","No","No","Internal","NOTED."]
[null,null,null,null,15118,"52_Tue Nov 24 2020 05:47:39 GMT+0000","2020-09-07","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","1 No. SOPEP drum was corroded, to be replaced with plastic drum.","LSA / FFA","Safety / LSA / FFA","External Factors","","","","","DRUM TO REPLACE.","2020-09-15","","Completed","2020-09-15","No","No","No","Internal","NOTED."]
[null,null,null,null,15119,"52_Tue Nov 24 2020 05:51:04 GMT+0000","2020-09-07","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Midship wilden pump suction and discharge hose is collapsible type. To be renewed with non-collapsible type.","Cargo Mach.","Cargo / Ballast Systems","Inappropriate Procedure","","","","","RENEW HOSE WITH SPARE NONCOLLAPSABLE HOSE.","2020-09-15","","Completed","2020-09-15","No","No","No","Internal","NOTED."]
[null,null,null,null,15122,"52_Tue Nov 24 2020 05:57:10 GMT+0000","2020-09-07","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","SOPEP inventory list for the month not updated.","LSA / FFA","Cert. & Docu.","Human Error","","","","","SOPEP INVENTORY TO UPDATE.","2020-09-15","","Completed","2020-09-15","No","No","No","Internal","NOTED."]
[null,null,null,null,15123,"52_Tue Nov 24 2020 06:02:13 GMT+0000","2020-09-07","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","De-rusting works to be done in Bay no. 5,4,3, 19 and also the frames and supports for catwalk","Deck - Machinery","General Appearance","Inappropriate Procedure","","","","","BAY FABRIC MAINTENANCE TO COMPLETED WITHIN TARGET TIME.","2020-12-07","","Completed","2020-10-30","No","No","No","Internal","DECK FABRIC MAINTENANCE IS CONTINUOUS JOB AND AREAS SHOULD BE ALLOCATED FOR IMPROVISATION AND PLAN TO BE MADE TO COMPLETE COATING AFTER GOOD PREPARATION."]
[null,null,null,null,15126,"52_Tue Nov 24 2020 06:05:29 GMT+0000","2020-09-07","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Rescue boat securing straps are deteriorating due to weather exposure, same to be renewed.","LSA / FFA","Safety / LSA / FFA","Inappropriate Procedure","","","","","STRAPS TO RENEW.","2020-09-15","","Completed","2020-09-15","No","No","No","Internal","CONDITION MONITORING/VET ROUNDS SHOUDL CAPTURE SUCH OBSERVATIONS FOLLOWED BY ACTIONS."]
[null,null,null,null,15171,"52_Tue Nov 24 2020 06:20:04 GMT+0000","2020-09-07","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Gymnasium equipments to be secured.","Accommodation","Safety / LSA / FFA","Inappropriate Procedure","","","","","TO SECURE GYM EQUIPMENT.","2020-09-15","","Completed","2020-09-15","No","No","No","Internal","NOTED."]
[null,null,null,null,15173,"52_Tue Nov 24 2020 06:23:21 GMT+0000","2020-09-07","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Pipe store to be arranged and secured well.","E/R - Pipes/ valves & fittings","General Appearance","Inappropriate Procedure","","","","","STORE TO ARRANGE.","2020-09-15","","Completed","2020-09-15","No","No","No","Internal","NOTED."]
[null,null,null,null,15179,"52_Tue Nov 24 2020 06:30:45 GMT+0000","2020-09-07","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Steering gear room floor to be painted and housekeeping to be done.","Deck - Machinery","General Appearance","Inappropriate Procedure","","","","","HOUSEKEEPING JOB.","2020-09-15","","Completed","2020-09-15","No","No","No","Internal","NOTED."]
[null,null,null,null,15180,"52_Tue Nov 24 2020 06:32:51 GMT+0000","2020-09-07","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Workshop and Engine room store to be cleaned and arranged.","Miscellaneous","General Appearance","Inappropriate Procedure","","","","","HOUSEKEEPING JOB","2020-09-15","","Completed","2020-09-15","No","No","No","Internal","NOTED."]
[null,null,null,null,15182,"52_Tue Nov 24 2020 06:45:16 GMT+0000","2020-09-07","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","MSBD, ESBD and local starter panel to be cleaned.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Inappropriate Procedure","","","","","HOUSEKEEPING JOB.","2020-09-15","","Completed","2020-09-15","No","No","No","Internal","NOTED."]
[null,null,null,null,15183,"52_Tue Nov 24 2020 06:49:13 GMT+0000","2020-09-07","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ME Cylinder oil tank top to be cleaned","E/R - Main Engine","General Appearance","Inappropriate Procedure","","","","","HOUSEKEEPING.","2020-09-15","","Completed","2020-09-15","No","No","No","Internal","ENSURE HOUSEKEEPING IN THIS AREA IS GOOD AS ANY OIL IS FIRE HAZARD."]
[null,null,null,null,15184,"52_Tue Nov 24 2020 06:51:15 GMT+0000","2020-09-07","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","A/E #2 crank case relief door leakage to be rectified","E/R - Aux. Engine","Eng. / Strg. Comp.","Inappropriate Procedure","","","","","LEAKAGE TO RECTIFY.","2020-09-15","","Completed","2020-09-15","No","No","No","Internal","NOTED."]
[null,null,null,null,15185,"52_Tue Nov 24 2020 06:54:25 GMT+0000","2020-09-07","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","A/E #2 fuel oil filter block leakage to be rectified.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","LEAKAGE RECTIFICATION.","2020-09-15","","Completed","2020-09-15","No","No","No","Internal","NOTED."]
[null,null,null,null,15186,"52_Tue Nov 24 2020 06:56:49 GMT+0000","2020-09-07","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Latest isolation form to be used in Engine Room","Documentation","Cert. & Docu.","Human Error","","","","","","2020-09-10","","Completed","2020-09-10","No","No","No","Internal","TO USE LATEST FORM ALWAYS."]
[null,null,null,null,15187,"52_Tue Nov 24 2020 07:00:51 GMT+0000","2020-09-07","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","AC expansion valve to be replaced","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","TO RENEW EXPANSION VALVE.","2020-11-15","","Completed","2020-10-30","No","No","No","Internal","NOTED THAT VALVE RENEWED AFTER RECEIPT OF SPARE."]
[null,null,null,null,14193,"52_06/10/2020 2:39:20 PM","2020-09-07","Observation","Ship Staff","Ship Staff Insp.","Derusting works to be done in bay no. 5, 4, 3, 19 and alos frames and supports for catwalk.","Miscellaneous","General Appearance","External Factors","11.3","Medium","","","Derusting work completed in bay no.5, 4, 3 and 19 completed","2020-12-07","","Completed","2020-10-26","No","No","No","Internal","WORK IN PROGRESS. TRY TO ACCOMPLISH IT BY SET TARGET."]
[null,null,null,null,14199,"52_06/10/2020 2:11:04 PM","2020-09-07","Observation","Ship Staff","Ship Staff Insp.","Bridge wing MOB marker ropes faded, to be renewed","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.31","High","","","Faded ropes renewed.","2020-09-14","","Completed","2020-09-08","No","No","No","Internal"]
[null,null,null,null,14200,"52_06/10/2020 2:12:37 PM","2020-09-07","Defect","Ship Staff","Ship Staff Insp.","Battery room door packing to be renewed.","Accommodation","General Appearance","Equipment Related","11.6","Medium","","","Door packing renewed.","2020-09-14","","Completed","2020-09-13","No","No","No","Internal"]
[null,null,null,null,14201,"52_06/10/2020 2:14:24 PM","2020-09-07","Observation","Ship Staff","Ship Staff Insp.","Shore gangway ropes faded and wearing out, to be renwed.","Miscellaneous","Safety / LSA / FFA","Equipment Related","5.47","Low","","","Shore gangway ropes renewed.","2020-09-14","","Completed","2020-09-09","No","No","No","Internal"]
[null,null,null,null,14202,"52_06/10/2020 2:16:58 PM","2020-09-07","Defect","Ship Staff","Ship Staff Insp.","One deck stand roller, found hard to turn, to be made free.","Deck - Pipe / Fittings","Mooring","Equipment Related","9.18","Low","","","Deck stand roller eased up and greased again.","2020-09-14","","Completed","2020-09-08","No","No","No","Internal"]
[null,null,null,null,14203,"52_06/10/2020 2:18:48 PM","2020-09-07","Observation","Ship Staff","Ship Staff Insp.","Void space manhole, stencil of enclosed space not made after maintainence work, stencil; to be put.","Miscellaneous","General Appearance","Inappropriate Procedure","5.15","Medium","","","Stencil work completed on freshly de- rusted and painted manhole covers.","2020-09-14","","Completed","2020-09-08","No","No","No","Internal"]
[null,null,null,null,14204,"52_06/10/2020 2:20:53 PM","2020-09-07","Observation","Ship Staff","Ship Staff Insp.","Vapour manifold bolts short in length, requisition raised for same. to be renewed once received","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","6.8","High","","","Short bolts renewed with correct length.","2020-12-07","","Completed","2020-09-12","No","No","No","Internal"]
[null,null,null,null,14205,"52_06/10/2020 2:22:50 PM","2020-09-07","Defect","Ship Staff","Ship Staff Insp.","One SOPEP drum was corroded, to be replaced with plastic drum.","Miscellaneous","MARPOL Related","Equipment Related","6.3","Low","","","Empty plastic drum painted, stenciled, and replaced defective drum.","2020-09-14","","Completed","2020-09-08","No","No","No","Internal"]
[null,null,null,null,14206,"52_06/10/2020 2:24:35 PM","2020-09-07","Observation","Ship Staff","Ship Staff Insp.","Midshp wilden pump suction and discharge hose is collapsable type, to be renewed with non collapsable type.","Miscellaneous","General Appearance","Equipment Related","11.5","Medium","","","Replaced with non collapsable type.","2020-09-14","","Completed","2020-09-07","No","No","No","Internal"]
[null,null,null,null,14207,"52_06/10/2020 2:25:48 PM","2020-09-07","Observation","Ship Staff","Ship Staff Insp.","SOPEP inventory list for the month not updated.","Miscellaneous","MARPOL Related","Inappropriate Procedure","6.1","Medium","","","Inventory updated.","2020-09-14","","Completed","2020-09-07","No","No","No","Internal"]
[null,null,null,null,14208,"52_06/10/2020 2:27:25 PM","2020-09-07","Defect","Ship Staff","Ship Staff Insp.","Rescue boat securing straps are deteriorating due to weather exposure. Same to be renewd.","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.28","Very High","","","securing straps renewed.","2020-09-14","","Completed","2020-09-09","No","No","No","Internal"]
[null,null,null,null,14210,"52_06/10/2020 2:29:14 PM","2020-09-07","Observation","Ship Staff","Ship Staff Insp.","Gymnasium equipments to be secured.","Accommodation","General Appearance","Inappropriate Procedure","11.13","Low","","","Equipments secured properly.","2020-09-14","","Completed","2020-09-07","No","No","No","Internal"]
[null,null,null,null,15181,"52_Tue Nov 24 2020 06:42:24 GMT+0000","2020-09-15","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Update MSDS for chemicals with the latest ones. Old one to be disposed.","Documentation","Cert. & Docu.","Human Error","","","","","MSDS TO REPLACE.","2020-09-15","","Completed","2020-09-15","No","No","No","Internal","ENSURE CORRECT MSDS ARE POSTED."]
[null,null,null,null,14209,"52_06/10/2020 2:30:57 PM","2020-09-21","Defect","Ship Staff","Ship Staff Insp.","During inspection of hydraullic hoses of miodship crane, five hoses were found to be deteriorating.","Deck - Machinery","Cargo / Ballast Systems","Equipment Related","8.5","Medium","","","All five hoses renewed.","2020-09-30","","Completed","2020-09-29","No","No","No","Internal"]
[null,null,null,null,14195,"52_7/10/2020 5:31:35 PM","2020-10-12","Observation","Ship Staff","Ship Staff Insp.","FWG Evaporator tubes need drilling for cleaning","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","recd drill bit. ","2021-04-15","EBAY210037 and EBAY210044","Completed","2021-02-01","No","No","No","Internal","Ordered Masonry/Concrete drill bits from Singapore and will be connected on board soon."]
[null,null,null,null,17867,"52_18/2/2021 9:49:08 AM","2020-11-01","Observation","Ship Staff","Ship Staff Insp.","Hose handling Limit Switch is malfunctional","Deck - Machinery,Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.5","Medium","","","spare recd","2021-04-05","EBAY200208","Completed","2021-02-20","No","No","No","Internal"]
[null,null,null,null,14191,"52_7/10/2020 5:23:52 PM","2020-11-30","Breakdown","Ship Staff","Ship Staff Insp.","MGPS STARBOARD SIDE ANODE WASTED","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","NEW ANODES FITTED","2021-02-28","EBAY200177","Completed","2021-02-14","No","No","No","Internal","ANODES ARE PROCURED AND IN PROCESS TO CONNECT ON BOARD."]
[null,null,null,null,16232,"52_18/12/2020 10:37:48 AM","2020-12-01","Observation","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","FW Temp Controller Found leaking","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","spares recd.","2021-02-15","EBAY200217","Completed","2021-02-20","No","No","No","External","NOTED THAT PRESENTLY LEAK IS STOPPED AND UNIT IS FUNCTIONING IN ORDER. SPARES UNDER EBAY200217 ARE ORDERED AND WILL BE CONNECTED ONCE READY."]
[null,null,null,null,16234,"52_19/12/2020 09:27:15","2020-12-01","Observation","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","Inspector Observations: Cargo Ship Safety Equipment Certificate (Form E) was wrongly emitted.\n\nQuestions:\n\n6.1 Those for which approved launching appliances are required.\n\n6.1.1 Number of liferafts was answered Two (2) instead One (1) onboard.\n\n6.2 Those for which approved launching appliances are not required.\n\n6.2.1 Number of liferafts was answered Two (2) instead One (1) onboard.\n\nRectified during the inspection, they received new certificate before inspector leave from the vessel","LSA / FFA","Cert. & Docu.","Human Error","2.1","Very High","","","Error notified to the office. In consultation with the class ABS office promptly arranged the new certificate with the rectification of the error. Same was inspected by the vetting inspector before leaving the vessel.\n\n","2020-12-01","","Completed","2020-12-01","No","No","No","External"]
[null,null,null,null,14192,"52_06/10/2020 2:37:09 PM","2020-12-11","Defect","Ship Staff","Ship Staff Insp.","During de-rusting work it was observed some parts of hawse pipe cover have thinned down","Miscellaneous","General Appearance","Equipment Related","11.5","Medium","","","Thinned down areas renewed. Hawse pipe covers de-rusted and painted.","2020-12-18","","Completed","2020-12-14","No","No","No","Internal","Noted the progress. Please complete the work in target period."]
[null,null,null,null,16231,"52_18/12/2020 10:35:32 AM","2020-12-15","Breakdown","Ship Staff","Ship Staff Insp.","pick up sensor of lubricator is defective","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Req Raised. NEW SENSOR FITTED","2021-01-31","EBAY200238","Completed","2021-02-15","No","No","No","Internal","EBAY200238 ordered and will be connected on board once spares are ready for dispatch."]
[null,null,null,null,null,"52_19/02/2021 12:57:25","2021-01-04","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Cable and hydraulic lines upporting tray under the catwalk is corrroded and wasted in some places,same to be renewed.","Deck - Pipe / Fittings","General Appearance","Equipment Related",11.4,"Very High","Not Applicable","Not Applicable","All supporting trays renewed.","2021-03-31",null,"Completed","2021-04-21","No",null,null,"Internal"]
[null,null,null,null,15131,"52_Tue Nov 24 2020 06:15:46 GMT+0000","2021-01-05","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Water fountain in the gymnasium not working, to be made functional.","Accommodation","MLC Related","Human Error,Equipment Related","12.8","High","","","WATER FOUNTAIN TO OPEN AND SERVICE TO MAKE IT OPERABLE.","2021-01-31","","Completed","2021-01-28","No","No","No","Internal","WATER FOUNTAIN - WATER LINES TO CHECK. CHECK IF REEFER COMP WORKS AND REPORT THE OUTCOME."]
[null,null,null,null,null,"52_19/2/2021 12:13:09 AM","2021-01-29","Breakdown","Ship Staff","Ship Staff Insp.","Laundary Heater not working","Accommodation","MLC Related","Equipment Related",12.8,"High","Not Applicable","Not Applicable","Spare part renewed and now working satisfactorily.","2021-03-29","EBAY210040","Completed","2021-04-10","No",null,null,"Internal"]
[null,null,null,null,null,"52_20/2/2021 4:32:37 PM","2021-02-05","Defect","Ship Staff","Ship Staff Insp.","water fountain in Engine room not functional","E/R - Pipes/ valves & fittings","MLC Related","Equipment Related",12.8,"High","Not Applicable","Not Applicable","new water purifier installed","2021-05-30",null,"Completed","2021-05-05","No",null,null,"Internal"]
[null,null,null,null,17866,"52_19/02/2021 14:11:28","2021-02-07","Defect","Ship Staff","Ship Staff Insp.","1S,2S,Slop Port COT IG branch valve worm gear weared off and not operational.","Miscellaneous","Cargo / Ballast Systems","Equipment Related","8.3","Medium","","","Requisition raised for spare valves.01 Old valve overhauled,assembled spare part from another old valves.","2021-03-25","EBAY210050","Completed","2021-03-01","No","No","No","Internal","Suggest to service/overhaul subject valves and needed new valves will be supplied next US call."]
[null,null,null,null,null,"52_01/05/2021 19:05:41","2021-02-07","Defect","Ship Staff","Ship Staff Insp.","3 Port COT IG branch valve worm gear weared off.","Cargo Mach.,Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related",8.3000000000000007,"Medium","Not Applicable","Not Applicable","Renewed with newly supply valve","2021-03-25",null,"Completed","2021-03-16","No",null,null,"Internal"]
[null,null,null,null,null,"52_18/2/2021 9:54:43 AM","2021-02-15","Defect","Ship Staff","Ship Staff Insp.","Toilet system malfunctions, flushing issue and flsuhing water issue in some cabin","Miscellaneous","MLC Related","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","spare received and toilet issue has been rectified","2021-04-04","EBAY210026","Completed","2021-04-08","No",null,null,"Internal"]
[null,null,null,null,null,"52_05/05/2021 02:01:30","2021-05-01","Observation","Ship Staff","Ship Staff Insp.","COT 2S Butterfly nut missing and other hexagonal nut used to tighten the tank dome.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related",8.3000000000000007,"Very High","Not Applicable","Not Applicable","Hexagonal nut to be replaced by proper size of butterfly nut.","2021-05-04",null,"Completed","2021-05-02","No",null,null,"Internal"]
[null,null,null,null,null,"52_5/5/2021 3:57:36 AM","2021-05-01","Defect","Ship Staff","Ship Staff Insp.","Observed atmospheric condenser sea water outlet pipe leakage.\t ","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related",10.31,"Very High","Not Applicable","Not Applicable","new pipe febricated and fitted back and tried out","2021-05-14",null,"Completed","2021-05-02","No",null,null,"Internal"]
[null,null,null,null,null,"52_05/05/2021 14:01:13","2021-05-02","Observation","Ship Staff","Ship Staff Insp.","One of the VRCS hydraulic line passing below catwalk found leaking","Deck - Pipe / Fittings","Cert. & Docu.","Equipment Related",8.3000000000000007,null,"Not Applicable","Not Applicable","Leakage was identified, found Ermeto coupling was loosen.Same was tightened and leak rectified.","2021-05-04",null,"Completed","2021-05-04","No",null,null,"Internal"]
[null,null,null,null,null,"52_5/5/2021 4:13:25 AM","2021-05-02","Observation","Ship Staff","Ship Staff Insp.","Lub oil purifier steam inlet valve to heater found leaking ","E/R - Boiler,E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related",10.31,"Very High","Not Applicable","Not Applicable","steam valve renewed","2021-05-05",null,"Completed","2021-05-03","No",null,null,"Internal"]
[null,null,null,null,null,"52_5/5/2021 4:23:05 AM","2021-05-03","Defect","Ship Staff","Ship Staff Insp.","AE #2 jacket water temperature sensor started malfunctioning and display showing reading error","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","Sensor renewed","2021-05-05",null,"Completed","2021-05-04","No",null,null,"Internal"]
[null,null,null,null,null,"52_06/06/2021 22:52:00","2021-06-03","Observation","Ship Staff","Ship Staff Insp.","Mid ship crane runner sheave not turning during operation","Deck - Machinery","Cargo / Ballast Systems","Equipment Related",8.5,"Medium","Not Applicable","Not Applicable","Overhauling and greasing of sheave carried out. Tested found satisfactory.","2021-06-15",null,"Completed","2021-06-10","No",null,null,"Internal"]
[null,null,null,null,null,"52_5/8/2021 10:09:19 AM","2021-06-28","Defect","Ship Staff","Ship Staff Insp.","Aux boiler gauge glass steam gasket  found leaking ","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related",null,null,"Not Applicable","Not Applicable","Gasket to be renew","2021-07-07",null,"Completed","2021-07-03","No",null,null,"Internal"]

{"sheet":"Calc","index":2,"n_rows":28,"n_cols":12,"rows_kept":28,"cut":false,"hidden":true,"merged":[]}
["Def_type","Def_cause","Equipments","VIQrefno","Observer_code"]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,"Dim itemSele As Long"]
[null,null,null,null,null,null,null,null,null,null,null,"   dim startRow as integer"]
[null,null,null,null,null,null,null,null,null,null,null,"   startRow=1"]
[null,null,null,null,null,null,null,null,null,null,null,"        For itemSele = 0 To ListBox1.ListCount - 1"]
[null,null,null,null,null,null,null,null,null,null,null,"        If ListBox1.Selected(itemSele) = True Then"]
[null,null,null,null,null,null,null,null,null,null,null,"        Worksheets(\"WorksheetName\").Range(\"A\" & startRow).Value = ListBox1.List(itemSele)"]
[null,null,null,null,null,null,null,null,null,null,null,"        startRow = startRow + 1"]
[null,null,null,null,null,null,null,null,null,null,null,"        End If"]
[null,null,null,null,null,null,null,null,null,null,null,"        Next"]
[null,null,null,null,null,null,null,null,null,null,null,"Dim LastRowA As String"]
[null,null,null,null,null,null,null,null,null,null,null,"        Dim itemSele As Long"]
[null,null,null,null,null,null,null,null,null,null,null,"       Dim startRow as integer"]
[null,null,null,null,null,null,null,null,null,null,null,"        LastRowA = ActiveSheet.Cells(Rows.count, \"A\").End(xlUp).row"]
[null,null,null,null,null,null,null,null,null,null,null,"        startQue = 0"]
[null,null,null,null,null,null,null,null,null,null,null,"        For itemSele = 0 To ListBox1.ListCount - 1"]
[null,null,null,null,null,null,null,null,null,null,null,"        For startRow = 1 To LastRowA"]
[null,null,null,null,null,null,null,null,null,null,null,"        If Worksheets(\"WorksheetName\").Range(\"A\" & startRow).Value = ListBox1.List(itemSele) Then"]
[null,null,null,null,null,null,null,null,null,null,null,"        ListBox1.Selected(itemSele) = True"]
[null,null,null,null,null,null,null,null,null,null,null,"        Exit For"]
[null,null,null,null,null,null,null,null,null,null,null,"        End If"]
[null,null,null,null,null,null,null,null,null,null,null,"        Next j"]
[null,null,null,null,null,null,null,null,null,null,null,"        Next"]
[null,null,null,null,null,null,null,null,null,null,null,"        End If"]

{"sheet":"Areaofobs","index":3,"n_rows":17,"n_cols":2,"rows_kept":17,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Cargo / Ballast Systems",11]
["Cert. & Docu.",2]
["Communication",6]
["Crew Management",3]
["Emgcy. Systems",13]
["Eng. / Strg. Comp.",14]
["General Appearance",15]
["Ice Opns.",17]
["ISM Related",7]
["ISPS Related",10]
["MARPOL Related",9]
["MLC Related",4]
["Mooring",12]
["Navigation",5]
["Safety / LSA / FFA",8]
["Structural Condn. / WT integrity ",16]

{"sheet":"Vessel_type","index":4,"n_rows":1,"n_cols":2,"rows_kept":1,"cut":false,"hidden":true,"merged":[]}
["Vessel_type","ID"]

{"sheet":"Deficiency_type","index":5,"n_rows":8,"n_cols":3,"rows_kept":8,"cut":false,"hidden":true,"merged":[]}
["TITLE","Type of deficiency_description","ID"]
["Breakdown",null,6]
["Critical Equipment",null,4]
["Defect",null,1]
["Guarantee Claim",null,8]
["Non Conformity",null,2]
["Observation",null,3]
["Other",null,7]

{"sheet":"VIQrefno","index":6,"n_rows":363,"n_cols":3,"rows_kept":363,"cut":false,"hidden":true,"merged":[]}
["VIQ_ref_no","Risk Value of observation","ID"]
["1.1","Low",8627]
["1.10","Low",8636]
["1.11","Low",8637]
["1.12","Low",8638]
["1.13","Low",8639]
["1.14","Low",8640]
["1.15","Low",8641]
["1.16","Low",8643]
["1.17","Low",8644]
["1.18","Low",8645]
["1.19","Low",8646]
["1.2","Low",8628]
["1.20","Low",8647]
["1.21","",8648]
["1.22","Low",8650]
["1.23","Low",8651]
["1.24","Low",8652]
["1.25","Low",8653]
["1.26","Low",8654]
["1.3","Low",8629]
["1.4","Low",8630]
["1.5","Low",8631]
["1.6","Low",8632]
["1.7","Low",8633]
["1.8","Low",8634]
["1.9","Low",8635]
["1.99","High",15785]
["10.1","Medium",8821]
["10.10","High",8830]
["10.11","Medium",8831]
["10.12","Very High",8832]
["10.13","Very High",8833]
["10.14","Medium",8834]
["10.15","Low",8835]
["10.16","Very High",8836]
["10.17","Very High",8837]
["10.18","High",8838]
["10.19","Very High",8839]
["10.2","Low",8822]
["10.20","High",8840]
["10.21","Medium",8841]
["10.22","Low",8842]
["10.23","Medium",8843]
["10.24","Low",8844]
["10.25","Very High",8845]
["10.26","High",8846]
["10.27","Medium",8847]
["10.28","Low",8848]
["10.29","Medium",8849]
["10.3","Medium",8823]
["10.30","High",8850]
["10.31","Very High",8851]
["10.32","Very High",8852]
["10.33","High",8853]
["10.34","High",8854]
["10.35","Very High",8855]
["10.36","Very High",8856]
["10.37","Medium",8857]
["10.38","Medium",8858]
["10.39","High",8859]
["10.4","High",8824]
["10.40","Medium",8860]
["10.41","Medium",8861]
["10.42","Medium",8862]
["10.43","Medium",8863]
["10.44","Medium",8864]
["10.45","Very High",8865]
["10.46","High",8866]
["10.47","Medium",8867]
["10.48","High",8868]
["10.49","Medium",8869]
["10.5","Low",8825]
["10.50","High",8870]
["10.51","Low",8871]
["10.52","Medium",8872]
["10.53","Medium",8873]
["10.54","High",8874]
["10.55","Low",8875]
["10.6","Very High",8826]
["10.7","Medium",8827]
["10.8","Medium",8828]
["10.9","Medium",8829]
["10.99","High",8876]
["11.1","High",8780]
["11.10","Medium",8789]
["11.11","Very High",8790]
["11.12","Low",8791]
["11.13","Low",8792]
["11.14","Medium",8793]
["11.15","Low",8794]
["11.16","Low",8795]
["11.17","Low",8796]
["11.2","Medium",8781]
["11.3","Medium",8782]
["11.4","Very High",8783]
["11.5","Medium",8784]
["11.6","Medium",8785]
["11.7","High",8786]
["11.8","Low",8787]
["11.9","Low",8788]
["11.99","High",8797]
["12.1","High",8798]
["12.10","High",8808]
["12.11","High",8809]
["12.12","High",8810]
["12.13","High",8811]
["12.14","High",8812]
["12.15","High",8813]
["12.16","High",8814]
["12.17","High",8815]
["12.18","High",8816]
["12.19","High",8817]
["12.2","High",8799]
["12.20","High",8818]
["12.21","High",8819]
["12.3","High",8801]
["12.4","High",8802]
["12.5","High",8803]
["12.6","High",8804]
["12.7","High",8805]
["12.8","High",8806]
["12.9","High",8807]
["12.99","High",8820]
["2.1","Very High",15]
["2.1.9","Very High",16]
["2.10","Medium",25]
["2.11","Medium",26]
["2.12","Medium",27]
["2.13","High",28]
["2.14","High",29]
["2.15","High",30]
["2.16","Medium",31]
["2.2","Medium",17]
["2.3","High",18]
["2.4","Medium",19]
["2.5","Low",20]
["2.6","Medium",21]
["2.7","High",22]
["2.8","Medium",23]
["2.9","Low",24]
["2.99","High",8672]
["3.1","High",8673]
["3.2","Very High",8674]
["3.3","High",8675]
["3.4","Low",8655]
["3.5","Medium",8676]
["3.6","High",8677]
["3.7","Very High",8678]
["3.8","Very High",8679]
["3.99","High",8680]
["4.1","High",8681]
["4.10","High",8690]
["4.11","Medium",8691]
["4.12","Very High",8692]
["4.13","Very High",8693]
["4.14","Very High",8694]
["4.15","Very High",8695]
["4.16","Very High",8696]
["4.17","Very High",8697]
["4.18","Very High",8698]
["4.19","Low",8699]
["4.2","Medium",8682]
["4.20","Very High",8700]
["4.21","High",8701]
["4.22","Low",8702]
["4.23","High",8703]
["4.24","High",8704]
["4.25","Low",8705]
["4.26","Low",8706]
["4.27","High",8707]
["4.3","Medium",8683]
["4.4","High",8684]
["4.5","Very High",8685]
["4.6","Medium",8686]
["4.7","High",8687]
["4.8","Medium",8688]
["4.9","Medium",8689]
["4.99","High",8708]
["5.1","Very High",8877]
["5.10","High",8886]
["5.11","Low",8887]
["5.12","Medium",8888]
["5.13","High",8889]
["5.14","Very High",8890]
["5.15","Medium",8891]
["5.16","Medium",8892]
["5.17","Very High",8893]
["5.18","High",8894]
["5.19","Medium",8895]
["5.2","Very High",8878]
["5.20","Medium",8896]
["5.21","Medium",8897]
["5.22","High",8899]
["5.23","Very High",8900]
["5.24","Very High",8901]
["5.25","Medium",8902]
["5.26","Medium",8903]
["5.27","Medium",8904]
["5.28","Very High",8905]
["5.29","High",8906]
["5.3","Low",8879]
["5.30","High",8907]
["5.31","High",8908]
["5.32","High",8909]
["5.33","High",8910]
["5.34","Low",8911]
["5.35","Medium",8912]
["5.36","Low",8913]
["5.37","Low",8914]
["5.38","High",8915]
["5.39","Very High",8916]
["5.4","High",8880]
["5.40","Very High",8917]
["5.41","Very High",8918]
["5.42","Medium",8919]
["5.43","High",8920]
["5.44","High",8921]
["5.45","Medium",8924]
["5.46","Medium",8925]
["5.47","Low",8926]
["5.48","Medium",8927]
["5.5","Low",8881]
["5.6","Low",8882]
["5.7","Medium",8883]
["5.8","Medium",8884]
["5.9","Very High",8885]
["5.99","High",8928]
["6.1","Medium",8709]
["6.10","Low",8718]
["6.11","High",8719]
["6.12","Medium",8720]
["6.13","Low",8721]
["6.14","High",8722]
["6.15","High",8723]
["6.16","Very High",8724]
["6.17","Very High",8725]
["6.18","Medium",8726]
["6.19","Low",8727]
["6.2","High",8710]
["6.20","Medium",8728]
["6.21","High",8729]
["6.22","Medium",8730]
["6.3","Low",8711]
["6.4","High",8712]
["6.5","Low",8713]
["6.6","Medium",8714]
["6.7","High",8715]
["6.8","High",8716]
["6.9","Low",8717]
["6.99","High",8731]
["7.1","High",8732]
["7.10","High",8741]
["7.11","High",8742]
["7.12","High",8743]
["7.13","Medium",8744]
["7.14","Medium",8745]
["7.15","High",8746]
["7.16","High",8747]
["7.17","High",8748]
["7.2","High",8733]
["7.3","Low",8734]
["7.4","Low",8735]
["7.5","Low",8736]
["7.6","Medium",8737]
["7.7","Low",8738]
["7.8","High",8739]
["7.9","High",8740]
["7.99","High",8749]
["8.1","Very High",8929]
["8.10","Very High",8938]
["8.11","Medium",8939]
["8.12","Medium",8940]
["8.13","Low",8941]
["8.14","Medium",8942]
["8.15","Medium",8943]
["8.16","Medium",8944]
["8.17","Medium",8945]
["8.18","Low",8946]
["8.19","Medium",8947]
["8.2","Medium",8930]
["8.20","Medium",8948]
["8.21","Medium",8949]
["8.22","Very High",8950]
["8.23","Medium",8951]
["8.24","Very High",8952]
["8.25","Medium",8953]
["8.26","Low",8954]
["8.27","Medium",8955]
["8.28","Medium",8956]
["8.29","Medium",8958]
["8.3","Medium",8931]
["8.30","Very High",8959]
["8.31","Medium",8960]
["8.32","Medium",8961]
["8.33","Very High",8962]
["8.34","High",8963]
["8.35","Medium",8964]
["8.36","Medium",8965]
["8.37","Medium",8967]
["8.38","Low",8968]
["8.39","Low",8969]
["8.4","Very High",8932]
["8.40","Very High",8970]
["8.41","Very High",8971]
["8.42","Medium",8972]
["8.43","Low",8973]
["8.44","Medium",8975]
["8.45","High",8976]
["8.46","Medium",8977]
["8.47","Medium",8978]
["8.48","Medium",8979]
["8.49","Medium",8980]
["8.5","Medium",8933]
["8.50","Very High",8981]
["8.51","Very High",8982]
["8.52","Very High",8983]
["8.53","Very High",8984]
["8.54","Medium",8985]
["8.55","Very High",15711]
["8.56","Very High",15712]
["8.57","Medium",15713]
["8.58","Medium",15714]
["8.59","Very High",15715]
["8.6","Medium",8934]
["8.60","Medium",15716]
["8.61","Low",15717]
["8.62","Medium",15718]
["8.63","Medium",15719]
["8.7","Very High",8935]
["8.8","Very High",8936]
["8.9","High",8937]
["8.99","High",15755]
["9.1","Low",8750]
["9.10","Medium",8759]
["9.11","Medium",8760]
["9.12","Medium",8761]
["9.13","Low",8762]
["9.14","Medium",8763]
["9.15","Medium",8764]
["9.16","High",8765]
["9.17","High",8766]
["9.18","Low",8767]
["9.19","Low",8768]
["9.2","Very High",8751]
["9.20","Medium",8769]
["9.21","Medium",8770]
["9.22","Low",8771]
["9.23","Low",8772]
["9.24","Medium",8773]
["9.25","Low",8774]
["9.26","Low",8775]
["9.27","Low",8776]
["9.28","Medium",8777]
["9.29","Low",8778]
["9.3","Very High",8752]
["9.4","High",8753]
["9.5","High",8754]
["9.6","Low",8755]
["9.7","Medium",8756]
["9.8","Medium",8757]
["9.9","Medium",8758]
["9.99","High",8779]

{"sheet":"Equipment_list","index":7,"n_rows":28,"n_cols":3,"rows_kept":28,"cut":false,"hidden":true,"merged":[]}
["TITLE","Equipment_list_description","ID"]
["Accommodation",null,12]
["Cargo Mach.",null,13]
["Critical Equip.",null,16]
["Deck - Machinery",null,18]
["Deck - Mooring Machinery",null,15]
["Deck - Pipe / Fittings",null,20]
["Documentation",null,21]
["E/R - Air Comp.",null,8]
["E/R - Aux. Engine",null,4]
["E/R - Aux. Mach.",null,7]
["E/R - Boiler",null,5]
["E/R - Main Engine",null,3]
["E/R - Pipes/ valves & fittings",null,9]
["E/R - Pumps",null,32]
["E/R - Purifier",null,6]
["Elect. Mach. & Equip.",null,10]
["Hull & Tanks",null,19]
["Inert Gas",null,14]
["LSA / FFA",null,17]
["Miscellaneous",null,22]
["Navigation - DGPS / EPFS / AIS",null,28]
["Navigation - ECDIS",null,25]
["Navigation - Echo Sounder / Speed Log",null,26]
["Navigation - GMDSS & Communication",null,23]
["Navigation - Others",null,11]
["Navigation - RADAR",null,24]
["Navigation - VDR / BNWAS",null,30]

{"sheet":"PSC_MOU","index":8,"n_rows":11,"n_cols":3,"rows_kept":11,"cut":false,"hidden":true,"merged":[]}
["TITLE","PSC_MOU_description","ID"]
["Asia and the Pacific",null,2]
["Caribbean",null,4]
["Europe and the North Atlantic",null,1]
["Latin America",null,3]
["The Black Sea region",null,6]
["The Indian Ocean",null,8]
["The Mediterranean",null,7]
["The Riyadh MoU",null,9]
["USCG",null,10]
["West and Central Africa",null,5]

{"sheet":"Inspection_type","index":9,"n_rows":13,"n_cols":2,"rows_kept":13,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Bunkering Audit",14]
["Cargo Audit",17]
["Engineering Audit",16]
["ISM Audit",2]
["ISPS Audit",3]
["IT Audit",10]
["MLC Audit",1]
["Mooring Audit",9]
["Nav Audit / Verification",8]
["Onboard Training",18]
["Ship Staff Insp.",15]
["Suptd. Insp.",13]

{"sheet":"Deficiency_Cause","index":10,"n_rows":8,"n_cols":3,"rows_kept":8,"cut":false,"hidden":true,"merged":[]}
["TITLE","Deficiency_Cause_description","ID"]
["Behaviour Based",null,1]
["Equipment Related",null,4]
["External Factors",null,5]
["Human Error",null,7]
["Inappropriate Procedure",null,8]
["Industry Issue",null,6]
["Knowledge Based",null,3]

{"sheet":"Observer_code","index":11,"n_rows":3,"n_cols":3,"rows_kept":3,"cut":false,"hidden":true,"merged":[]}
["TITLE","Observer_code_description","ID"]
["Owner / Marine / Tech. Suptd.",null,3]
["Ship Staff",null,2]

{"sheet":"Status_code","index":12,"n_rows":6,"n_cols":3,"rows_kept":6,"cut":false,"hidden":true,"merged":[]}
["TITLE","Status_code_description","ID"]
["Completed",null,6]
["Deferred to D D",null,5]
["In progress",null,3]
["Not Started",null,2]
["Waiting spare",null,4]

{"sheet":"PSC_ref_no","index":13,"n_rows":19,"n_cols":2,"rows_kept":19,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Alarms",9]
["Cargo operations including equipment",7]
["Certificates & Documentation",2]
["Dangerous Goods",13]
["Emergency Systems",5]
["Fire safety",8]
["ISM",16]
["ISPS",17]
["Life saving appliances",12]
["MLC, 2006",18]
["Other",19]
["Pollution Prevention",15]
["Propulsion and auxiliary machinery",14]
["Radio communication",6]
["Safety of Navigation",11]
["Structural condition",3]
["Water/Weathertight condition",4]
["Working and Living Conditions",10]

{"sheet":"Risk_value_of_obs","index":14,"n_rows":1,"n_cols":2,"rows_kept":1,"cut":false,"hidden":true,"merged":[]}
["Risk Value of observation","ID"]

{"sheet":"Year","index":15,"n_rows":18,"n_cols":1,"rows_kept":18,"cut":false,"hidden":true,"merged":[]}
["Year"]
[2014]
[2015]
[2016]
[2017]
[2018]
[2019]
[2020]
[2021]
[2022]
[2023]
[2024]
[2025]
[2026]
[2027]
[2028]
[2029]
[2030]

{"sheet":"Month","index":16,"n_rows":13,"n_cols":1,"rows_kept":13,"cut":false,"hidden":true,"merged":[]}
["Month"]
["Jan"]
["Feb"]
["Mar"]
["Apr"]
["May"]
["Jun"]
["Jul"]
["Aug"]
["Sep"]
["Oct"]
["Nov"]
["Dec"]

{"sheet":"Date_","index":17,"n_rows":32,"n_cols":1,"rows_kept":32,"cut":false,"hidden":true,"merged":[]}
["Date"]
["01"]
["02"]
["03"]
["04"]
["05"]
["06"]
["07"]
["08"]
["09"]
[10]
[11]
[12]
[13]
[14]
[15]
[16]
[17]
[18]
[19]
[20]
[21]
[22]
[23]
[24]
[25]
[26]
[27]
[28]
[29]
[30]
[31]

{"sheet":"Sheet1","index":18,"n_rows":24,"n_cols":6,"rows_kept":24,"cut":false,"hidden":true,"merged":[]}
[]
[null,"ID","E",null,"Date Recorded",1]
[null,"UNIQUE ID","F",null,"Type of Deficiency",2]
[1,"Date Recorded","G",null,"Observer code",3]
["ignore","Vessel Type","H",null,"Type of Inspection",4]
[null,"Internal / External","I",null,"Description of Deficiency",5]
[null,"Drydock","J",null,"Equipment Categories",6]
[null,"Information Sharing","K",null,"Area of Observation",7]
[null,"Critical_item","L",null,"Deficiency Cause",8]
[null,"Deficiency Type","M",null,"VIQ Ref Number",9]
[null,"Deficiency Cause","N",null,"Risk Value of Obs",10]
[null,"Inspection Type","O",null,"PSC Ref Number",11]
[null,"Equipments","P",null,"PSC MOU ID",12]
[null,"VIQ Reference Number","Q",null,"Action Taken or Required",13]
[null,"Risk Value of the observation","R",null,"Target Date",14]
[null,"PSC Reference Number","S",null,"PO Ref No.",15]
[null,"PSC MOU","T",null,"Status Code",16]
[null,"Observer Code","U",null,"Date Completed",17]
[null,"Target Date","V",null,"Drydock",18]
[null,"Status Code","W",null,"Info Sharing",19]
[null,"Description of Deficiency","X",null,"Critical Item Flag",20]
[null,"Action taken / required","Y",null,"Audit Type",21]
[null,"PO ref no","Z"]
[null,"Date completed","AA"]

{"sheet":"Ship_information","index":19,"n_rows":2,"n_cols":3,"rows_kept":2,"cut":false,"hidden":true,"merged":[]}
["Ship_ID","Ship_Name","FILE_NAME"]
["52","EAGLE BAY (28-02-2021)","52_1619684199561.xlsm"]

{"sheet":"External_Deficiency_type","index":20,"n_rows":5,"n_cols":3,"rows_kept":5,"cut":false,"hidden":true,"merged":[]}
["TITLE","Type of deficiency_description","ID"]
["Condn of Class / Memo",null,5]
["Defect",null,1]
["Non Conformity",null,2]
["Observation",null,3]

{"sheet":"External_Inspection_type","index":21,"n_rows":11,"n_cols":2,"rows_kept":11,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Cargo Audit",17]
["Flag State Insp.",5]
["ISM Audit",2]
["ISPS Audit",3]
["MLC Audit",1]
["Nav Audit / Verification",8]
["OM Insp. (Eg. SIRE / CDI etc.)",6]
["Others (Eg. Insurance etc.)",12]
["PSC Inspection",4]
["Terminal Insp.",11]

{"sheet":"External_Observer_code","index":22,"n_rows":7,"n_cols":3,"rows_kept":7,"cut":false,"hidden":true,"merged":[]}
["TITLE","Observer_code_description","ID"]
["Class Surveyor",null,4]
["FSC Inspector",null,5]
["Others (Eg. Insurance etc.)",null,9]
["PSC Insp.",null,6]
["SIRE / CDI Insp.",null,8]
["Terminal Insp.",null,7]

{"sheet":"Sheet Version","index":23,"n_rows":2,"n_cols":2,"rows_kept":2,"cut":false,"hidden":true,"merged":[]}
["Version","Title"]
["2.0","Version 2.0"]