{"text_format":"1","workbook":"xlsx","n_sheets":24,"sheets":["Mainsheet","Completed","Calc","Areaofobs","Vessel_type","Deficiency_type","VIQrefno","Equipment_list","PSC_MOU","Inspection_type","Deficiency_Cause","Observer_code","Status_code","PSC_ref_no","Risk_value_of_obs","Year","Month","Date_","Sheet1","Ship_information","External_Deficiency_type","External_Inspection_type","External_Observer_code","Sheet Version"],"not_rendered":{"charts":0,"images":5,"macros":1,"external_links":0,"defined_names":12,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Mainsheet","index":0,"n_rows":32,"n_cols":28,"rows_kept":32,"cut":false,"hidden":false,"merged":[[10,8,10,9],[10,12,10,13],[12,6,12,27],[8,6,8,27]]}
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,"Defect - Damage Monitoring Sheet"]
[]
[null,null,null,null,null,null,null,"Date of Report","02-Dec-2021",null,null,"Ship Name","DHT HAWK (02-12-2021)"]
[]
[null,null,null,null,null,null,"VERSION : 2.0"]
[]
[]
[]
[null,null,null,null,"ID","UNIQUE ID","Date Recorded","Type of Deficiency","Observer code","Type of Inspection","Description of Deficiency","Equipment Categories","Area of Observation","Deficiency Cause","VIQ Ref Number","Risk Value of Obs","PSC Ref Number","PSC MOU ID","Action Taken or Required","Target Date","PO Ref No.","Status Code","Date Completed","Drydock","Info Sharing","Critical Item","Audit Type","Superintendent Remarks"]
[null,null,null,null,19920,"23_17/05/2021 9:11:29 PM","2021-09-12","Observation","Ship Staff","Ship Staff Insp.","5 P & 5 S COT valve indicator potentiometer in CCR panel faulty","Cargo Mach.","Cargo / Ballast Systems","Equipment Related",8.8000000000000007,"Medium","Not Applicable","Not Applicable","Need to replace the faulty potentiometer","2022-01-31","DHAW210145","Waiting spare",null,"No","No","No","Internal","spares awaiting connection"]
[null,null,null,null,22003,"23_24/10/2021 11:46:40 PM","2021-09-24","Defect","Ship Staff","Ship Staff Insp.","EGCS- Exh.gas emission monitoring system faulty.","Miscellaneous","MARPOL Related","Equipment Related","9.28","Medium","","","Job is in progress, Technician follow-up messages is in progress.","2021-12-15","","In progress",null,"No","No","No","Internal","CEMS spares confirmed and service to be arranged again at next port where tech can be engaged."]
[null,null,null,null,21348,"23_01/10/2021 11:46:22 AM","2021-09-30","Observation","Ship Staff","Ship Staff Insp.","Provision crane jib top end & hook block sheaves were found with larger depth than the jib inner sheave","Deck - Machinery","ISM Related","Equipment Related",8.5,"Very High","Not Applicable","Not Applicable","Sheave & centre pin removed & inspected. No damages to pin & sheave brearing. Depth of sheave channel larger than other sheaves. Suggest to renew the same at next oppertunity","2022-01-31","DHAW210284","Waiting spare",null,"No","No","No","Internal","spares processed for supply"]
[null,null,null,null,21598,"23_04/10/2021 1:19:59 PM","2021-10-03","Observation","Ship Staff","Ship Staff Insp.","BW-V 813: No 1 ballast pump discharge valve body has a pin hole leak. Soft repair carried out. ","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related",8.11,"Medium","Not Applicable","Not Applicable","Valve to be replaced. New spare ordered.","2022-01-31","DHAW210292","Waiting spare",null,"No","No","No","Internal","complete as planned and close out. check after inspection if we need to renew the valve"]
[null,null,null,null,21599,"23_04/10/2021 1:22:13 PM","2021-10-03","Observation","Ship Staff","Ship Staff Insp.","BW-V 831 No 2 ballast p/p sea chest valve- Actuator leaking when CLOSE command given due to wear on actuator piston","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related",8.11,"Medium","Not Applicable","Not Applicable","Valve to be replaced. Requisition for new Valve raised in PAL.","2022-01-30","DHAW210292","Waiting spare",null,"No","No","No","Internal","noted ; revert with the spares requirement if any and include the RO number in the sheet"]
[null,null,null,null,22007,"23_22-Oct-21 14:51:08","2021-10-19","Observation","Ship Staff","Ship Staff Insp.","BHC Test kit Hyd. Jack not on board.","Deck - Mooring Machinery","Mooring","Equipment Related",9.14,"Medium","Not Applicable","Not Applicable","Requisition for same raised.DHAW210288","2022-01-31","DHAW210288","In progress",null,"No","No","No","Internal","spares confirmed for supply, to be connected once ready"]
[null,null,null,null,22014,"23_23/10/2021 10:54:40 AM","2021-10-20","Defect","Ship Staff","Ship Staff Insp.","Valve indicator not working for Valves : COV924,COV915,COV905,COV508, SRV911 andSRV924.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related",8.8000000000000007,"Medium","Not Applicable","Not Applicable","To be rectified.","2022-01-31",null,"In progress",null,"No","No","No","Internal","please plan and close out on priority; check the spares and revert if any additional required. include job in DDRL, if unable to close out by end DEC"]
[null,null,null,null,22015,"23_23/10/2021 11:43:41 am","2021-10-20","Defect","Ship Staff","Ship Staff Insp.","Stbd. hose handling crane hyd. Motor to be replaced. Spare motor on board and will be carried out when there is suitable opportunity/ weather condition. \n\nAlso Stbd. hose handling crane limit switch sluggish. To be rectified.","Cargo Mach.,Deck - Machinery","Cargo / Ballast Systems","Equipment Related",8.5,"Very High","Not Applicable","Not Applicable","Motor onboard, to be changed. \nmotor in place is good and reliable for use - issue is slight slow in operation ( working well on high torque and slow speed)","2022-01-31",null,"Not Started",null,"No","No","No","Internal","complete on priority  and close out."]
[null,null,null,null,22685,"23_04/11/2021 9:01:15 AM","2021-10-21","Critical Equipment","Ship Staff","Ship Staff Insp.","During routine ODME tests, noted that the sampling pump is running continously in Auto mode, even when the ODME power is OFF. Sampling Pump mechanical seal found leaking.","Critical Equip.","MARPOL Related","Equipment Related",6.13,"Low","Not Applicable","Not Applicable","Operation satisfactory, leaking seal to be replaced","2022-01-31","DHAW210309","In progress",null,"No","No","No","Internal","pump reapirs managed by teflon seal fabricated onboard.\nspares confirmed for supply and to be connected at next available port."]
[null,null,null,null,22686,"23_4/11/2021 11:11:31 am","2021-10-24","Defect","Ship Staff","Ship Staff Insp.","STBD gangway does not stow fully near davit and has to be stowed and unstowed using a chain block, the control of slewing is by direct connection to the air motor.","Deck - Pipe / Fittings","Safety / LSA / FFA","Equipment Related",5.47,"Medium","Not Applicable","Not Applicable","Renewed one of the wasted line, other line and 3 way valve to be fitted, vsl does not have thread die to carry out the job.","2022-01-31",null,"In progress",null,"No","No","No","Internal","raise RO for required tools to complete the job. and include in DDRL in case unable to resolve."]
[null,null,null,null,22687,"23_4/11/2021 11:14:29 am","2021-10-24","Defect","Ship Staff","Ship Staff Insp.","Port gangway cannot be operated from the control position, both hoisting and slewing air motor to be directly connected to operate.","Deck - Pipe / Fittings","Safety / LSA / FFA","Equipment Related",5.47,"Medium","Not Applicable","Not Applicable","One of the leaking lines renewed, vsl does not have thread die to carry out remaining repairs.","2022-01-31",null,"In progress",null,"No","No","No","Internal","raise RO for the required spares and tools to complete the job"]
[null,null,null,null,null,null,"2021-12-17","Observation","Ship Staff","Ship Staff Insp.","M/E LUB.OIL PURIFIER DUE FOR MAJOR OVERHAUL.","E/R - Purifier","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","PRESENT PERFORMANCE IS SATISFACTORY. PLAN TO CARRYOUT THE MAINTENANCE AFTER DISCHARGE PORT.","2022-01-15",null,"Not Started",null,"No",null,null,"Internal"]
[null,null,null,null,null,null,"2021-12-20","Defect","Ship Staff","Ship Staff Insp.","M/E LUB.OIL COOLER S.W.IN/OUT PIPES,MINOR SEA WATER LEAKAGE. PIPES TO BE RENEWED.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","PIPE FABRIATION IS IN PROGRESS.","2022-01-15",null,"In progress",null,"No",null,null,"Internal"]
[null,null,null,null,null,"23_03/01/2022 11:57:03 AM","2021-12-26","Defect","Ship Staff","Ship Staff Insp.","Mooring winch MW1, MW2, MW7 having minor leak from operation control block.","Deck - Machinery","Mooring","Equipment Related",9.14,"Medium","Not Applicable","Not Applicable","To be rectified","2022-01-31",null,"In progress",null,"No",null,null,"Internal"]
[null,null,null,null,null,null,"2021-12-26","Defect","Ship Staff","Ship Staff Insp.","MINOR WATER LEAKAGE FOR NO.1 BOILER PREHEATING CONDENSATE RETURN LINE.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related",10.32,"Very High","Not Applicable","Not Applicable","VALVES WERE NOT HOLDING. PLAN OVERHAUL VALVE AND REPLACE GASKET.","2022-01-15",null,"Not Started",null,"No",null,null,"Internal"]

{"sheet":"Completed","index":1,"n_rows":715,"n_cols":28,"rows_kept":715,"cut":false,"hidden":false,"merged":[[10,8,10,9],[10,12,10,13],[12,6,12,27],[8,6,8,27]]}
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,"Defect - Damage Monitoring Sheet"]
[]
[null,null,null,null,null,null,null,"Date of Report","02-Dec-2021",null,null,"Ship Name","DHT HAWK (02-12-2021)"]
[]
[null,null,null,null,null,null,"VERSION : 2.0"]
[]
[]
[]
[null,null,null,null,"ID","UNIQUE ID","Date Recorded","Type of Deficiency","Observer code","Type of Inspection","Description of Deficiency","Equipment Categories","Area of Observation","Deficiency Cause","VIQ Ref Number","Risk Value of Obs","PSC Ref Number","PSC MOU ID","Action Taken or Required","Target Date","PO Ref No.","Status Code","Date Completed","Drydock","Info Sharing","Critical Item","Audit Type","Superintendent Remarks"]
[null,null,null,null,3351,"23_2019-07-07 14:54:19.995","2018-08-21","Defect","Ship Staff","Ship Staff Insp.","M/E Viscotherm leaking from seal","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Seal renewed with new spare.","2019-04-30","DHAW190006","Completed","2019-03-20","No","No","No","Internal"]
[null,null,null,null,3384,"23_2019-10-02 05:59:28.000","2018-08-29","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Pilot Cabin Port Hole has Silicon Patch","Accommodation","General Appearance","Equipment Related","","","","","ORDERED NEW, AWAITING SPARE.","2019-07-28","DHAW180301","Completed","2019-07-25","No","No","No","Internal"]
[null,null,null,null,3337,"23_2019-08-24 14:54:19.995","2018-09-14","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Appearance of thick and old paint; valves are jammed. Remove the thick paint and ease off the valves","Deck - Pipe / Fittings","General Appearance","Equipment Related","","","","","Hydro blasted & repainted. All COW, IG branch,Pumproom valves,manifold v/v greased, freed, excessive paint removed.","2019-03-13","","Completed","2019-03-15","No","No","No","Internal"]
[null,null,null,null,3289,"23_2019-09-06 14:54:20.000","2018-09-22","Defect","Ship Staff","Ship Staff Insp.","IG line pressure gauge on bridge defective ","Inert Gas","General Appearance","Equipment Related","","","","","Inspected the same found the pressure to be same as other places. Adjusted the mechanism of pressure gauge needle and made operational.","2018-12-22","DHAW180242","Completed","2019-01-13","No","No","No","Internal"]
[null,null,null,null,3376,"23_2019-06-02 14:54:19.995","2018-10-19","Defect","Ship Staff","Ship Staff Insp.","HFO FO Service tank level gauge not operational","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Received level gauge is defective","2019-06-30","DHAW180253","Completed","2019-06-28","No","No","No","Internal"]
[null,null,null,null,3361,"23_2019-07-17 14:54:19.995","2018-11-03","Defect","Ship Staff","Ship Staff Insp.","Aux.boiler FO burn pump No.2 mechanical seal leaking","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","New pump received and installed.","2019-04-30","DHAW190018","Completed","2019-05-04","No","No","No","Internal"]
[null,null,null,null,3311,"23_2019-09-28 14:54:20.000","2018-11-04","Defect","Ship Staff","Ship Staff Insp.","Alpha lubricator tacho pickup faulty","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Spare received and pick-up renewed.","2018-12-03","DHAW180296","Completed","2019-02-13","No","No","No","Internal"]
[null,null,null,null,3290,"23_2019-09-07 14:54:20.000","2018-11-10","Defect","Ship Staff","Ship Staff Insp.","Forward mast Air horn heater defective showing low insulation, heater presently isolated","Elect. Mach. & Equip.","General Appearance","Equipment Related","","","","","Heater and terminal box replaced with received new spares","2018-12-09","DHAW180273","Completed","2019-01-28","No","No","No","Internal"]
[null,null,null,null,3291,"23_2019-09-08 14:54:20.000","2018-11-15","Defect","Ship Staff","Ship Staff Insp.","\"Input\" Button on the Controller Keypad (ODME) not working","Critical Equip.","General Appearance","Equipment Related","","","","","Keypad replaced with new spare","2019-01-25","DHAW180292","Completed","2019-01-27","No","No","No","Internal"]
[null,null,null,null,3312,"23_2019-09-29 14:54:20.000","2018-12-05","Defect","Ship Staff","Ship Staff Insp.","#3 MAC after cooler tube leaking","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related","","","","","New spare cooler received and renewed.","2019-01-20","DHAW180297","Completed","2019-02-19","No","No","No","Internal"]
[null,null,null,null,3309,"23_2019-09-26 14:54:20.000","2018-12-14","Defect","Ship Staff","Ship Staff Insp.","2 Nos. JRC two -way VHF Radiotelephone not working-Model-JHS-7 ,Serial Nos. BV 71307 & BV 71305","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","Completed","2019-12-31","DHAW180300","Completed","2019-12-16","No","No","No","Internal"]
[null,null,null,null,3313,"23_2019-09-30 14:54:20.000","2018-12-28","Defect","Ship Staff","Ship Staff Insp.","#2 Boiler water circulating pump needs overhauling. Throttle bush and sleeve clearance is above limits","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Spares received. Throttle bush renewed.","2019-01-31","DHAW190012","Completed","2019-02-08","No","No","No","Internal"]
[null,null,null,null,3357,"23_2019-07-13 14:54:19.995","2018-12-29","Defect","Ship Staff","Ship Staff Insp.","#2 EGE feed pump not developing sufficient pressure","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Root-cause found on Boiler water circulating pump throttle bush. After overhauling, pump started developing good pressure.","2019-04-30","DHAW190029","Completed","2019-03-19","No","No","No","Internal"]
[null,null,null,null,3314,"23_2019-08-01 14:54:19.999","2018-12-30","Defect","Ship Staff","Ship Staff Insp.","Fresh water tank valve not holding","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Valve overhauled and repaired.","2019-01-31","DHAW190006","Completed","2019-02-07","No","No","No","Internal"]
[null,null,null,null,3333,"23_2019-08-20 14:54:19.995","2018-12-31","Defect","Ship Staff","Ship Staff Insp.","Centrifugal filter body developed hair line crack","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Repair carried out onboard by Aluminium Welding.","2019-03-13","","Completed","2019-03-01","No","No","No","Internal"]
[null,null,null,null,3304,"23_2019-09-21 14:54:20.000","2019-01-05","Defect","Ship Staff","Ship Staff Insp.","Port side hose handling crane jib pin frozen","Deck - Machinery","General Appearance","Equipment Related","","","","","Awaiting shore assistance and spares","2019-02-05","DHAW190011","Completed","2019-02-09","No","No","No","Internal"]
[null,null,null,null,3375,"23_2019-06-01 14:54:19.999","2019-01-06","Defect","Ship Staff","Ship Staff Insp.","ME LO backwash filter diaphragm cracked and leaking","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Replaced with spare diaphram(fabricated spare) supplied by HaiTong Marine.","2019-06-30","DHAW190028","Completed","2019-06-22","No","No","No","Internal"]
[null,null,null,null,3292,"23_2019-09-09 14:54:20.000","2019-01-11","Defect","Ship Staff","Ship Staff Insp.","COPT #1 trips without any alarm when raised to 900 rpm","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","Relays 2A and 14C replaced as these are keep relays. To be monitored during discharge","2019-02-05","","Completed","2019-01-18","No","No","No","Internal"]
[null,null,null,null,3310,"23_2019-09-27 14:54:20.000","2019-01-12","Defect","Ship Staff","Ship Staff Insp.","Bridge front access door (STBD SIDE) hinges broken","Accommodation","General Appearance","Equipment Related","","","","","Need hot work","2019-02-28","","Completed","2019-02-20","No","No","No","Internal"]
[null,null,null,null,3364,"23_2019-07-20 14:54:19.995","2019-01-13","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Upper deck alley way walls to paint white upto tubelight level","Accommodation","General Appearance","Equipment Related","","","","","paints received. Will be tried out in loaded passage.","2019-04-20","DHAW190010","Completed","2019-04-22","No","No","No","Internal"]
[null,null,null,null,3366,"23_2019-07-22 14:54:19.995","2019-01-13","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","440 low insulation meter is sticky on one side; requ for new to raise and keep in stock","Elect. Mach. & Equip.","General Appearance","Equipment Related","","","","","Requisition raised. Old unit is working however, it sometimes needle stick on one side. Still awaiting to receive the new spare unit in order to replace.","2019-05-20","DHAW190035","Completed","2019-05-26","No","No","No","Internal"]
[null,null,null,null,3367,"23_2019-07-23 14:54:19.995","2019-01-13","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Port gangway aft sliding rail slight bent at one place to be straightened","Hull & Tanks","General Appearance","Equipment Related","","","","","COMPLETED","2019-05-20","","Completed","2019-05-30","No","No","No","Internal"]
[null,null,null,null,3368,"23_2019-07-24 14:54:19.995","2019-01-13","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","AE #2 exh line bellow on ECR flat sign of leakage","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","To create job in REFMAN. Requisition raised.","2019-05-01","","Completed","2019-06-01","No","No","No","Internal"]
[null,null,null,null,3369,"23_2019-07-25 14:54:19.995","2019-01-13","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Some crew and Jr officers cabin sofa has worn look. Raise RO for prefabricated covers","Accommodation","General Appearance","Equipment Related","","","","","some crew cabins sofa covered with old blankets & sheets. Collecting more blankets & sheets. Covering again Will be carried out at next opportunity. Requisition will be raised for prefabricated covers if short of old blankets & sheets .","2019-05-31","","Completed","2019-05-31","No","No","No","Internal"]
[null,null,null,null,3370,"23_2019-07-26 14:54:19.995","2019-01-13","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","AE control panel and meters panel on top of engine, cushy mountings to renew","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Requisition raised","2019-05-20","DHAW190043","Completed","2019-05-29","No","No","No","Internal"]
[null,null,null,null,3371,"23_2019-07-27 14:54:19.995","2019-01-13","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Damaged drawers and rails to repair","Accommodation","General Appearance","Equipment Related","","","","","COMPLETED","2019-05-13","","Completed","2019-06-01","No","No","No","Internal"]
[null,null,null,null,3380,"23_2019-06-06 14:54:19.995","2019-01-13","Defect","Ship Staff","Ship Staff Insp.","#1, #2 & #3 COPT governor valve stem bush threads damaged","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","No.1 Copt valve stem bush renewed with original supplied by Maker,No.2 & 3 found in good condition.","2019-06-16","DHAW190044","Completed","2019-06-15","No","No","No","Internal"]
[null,null,null,null,6709,"23_Sun Sep 01 2019 14:54:20 GMT+0000 (Coordinated Universal Time)","2019-01-13","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Damaged gratings to remove and the one with the flat bars missing in sides to provide with flat bar on all the four sides","Hull & Tanks","General Appearance","Equipment Related","11.5","Medium","","","Completed","2019-01-16","","Completed","2019-01-15","No","No","No","Internal"]
[null,null,null,null,6710,"23_Mon Sep 02 2019 14:54:20 GMT+0000 (Coordinated Universal Time)","2019-01-13","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Lifeboat stowing gripe wires to remove clean and grease. If condition is not satisfactory, then they must be replaced.","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.28","Very High","","","Completed","2019-01-27","","Completed","2019-01-16","No","No","No","Internal"]
[null,null,null,null,6711,"23_Tue Sep 03 2019 14:54:20 GMT+0000 (Coordinated Universal Time)","2019-01-13","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Port bridge door gasket detached at one corner, to stick or check if new gasket required","Accommodation","General Appearance","Equipment Related","8.29","High","","","Completed","2019-02-13","","Completed","2019-01-15","No","No","No","Internal"]
[null,null,null,null,6712,"23_Wed Sep 04 2019 14:54:20 GMT+0000 (Coordinated Universal Time)","2019-01-13","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Few tank radar protective canvas covers were torn, to replace with new canvas covers","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","11.7","High","","","Completed","2019-01-27","","Completed","2019-01-15","No","No","No","Internal"]
[null,null,null,null,3284,"23_2019-09-01 14:54:20.000","2019-01-13","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Damaged gratings to remove and the one with the flat bars missing in sides to provide with flat bar on all the four sides","Hull & Tanks","General Appearance","Equipment Related","","","","","Completed","2019-01-16","","Completed","2019-01-15","No","No","No","Internal"]
[null,null,null,null,3285,"23_2019-09-02 14:54:20.000","2019-01-13","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Lifeboat stowing gripe wires to remove clean and grease. If condition is not satisfactory, then they must be replaced.","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","Completed","2019-01-27","","Completed","2019-01-16","No","No","No","Internal"]
[null,null,null,null,3286,"23_2019-09-03 14:54:20.000","2019-01-13","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Port bridge door gasket detached at one corner, to stick or check if new gasket required","Accommodation","General Appearance","Equipment Related","","","","","Completed","2019-02-13","","Completed","2019-01-15","No","No","No","Internal"]
[null,null,null,null,3287,"23_2019-09-04 14:54:20.000","2019-01-13","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Few tank radar protective canvas covers were torn, to replace with new canvas covers","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","Completed","2019-01-27","","Completed","2019-01-15","No","No","No","Internal"]
[null,null,null,null,3288,"23_2019-09-05 14:54:20.000","2019-01-13","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Valve leaking, to overhaul and also the area below the drain valve to paint","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","Completed","2019-01-14","","Completed","2019-01-15","No","No","No","Internal"]
[null,null,null,null,3293,"23_2019-09-10 14:54:20.000","2019-01-13","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Lifeboat hose proper storing place and the spare to be kept in one box","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","Wooden box prepared, painted, stenciled and hose kept.","2019-01-20","","Completed","2019-01-28","No","No","No","Internal"]
[null,null,null,null,3294,"23_2019-09-11 14:54:20.000","2019-01-13","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Hot water circulating pump leaking gland packing to renew","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Gland packing renewed and leak rectified","2019-02-13","","Completed","2019-01-14","No","No","No","Internal"]
[null,null,null,null,3295,"23_2019-09-12 14:54:20.000","2019-01-13","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ME camshaft LO pump leaking from seal to repair ","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Gland packing nipped up and drain collecting box cleared. Leak rectified","2019-01-20","","Completed","2019-01-14","No","No","No","Internal"]
[null,null,null,null,3296,"23_2019-09-13 14:54:20.000","2019-01-13","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Accommodation ventilation checklist to prepare covering all the air dampers and flaps","Accommodation","General Appearance","Equipment Related","","","","","List prepared and posted in CCR, Ship's office & \n\nbridge.","2019-02-13","","Completed","2019-02-02","No","No","No","Internal"]
[null,null,null,null,3298,"23_2019-09-15 14:54:20.000","2019-01-13","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Stbd crane stand one rail broken","Deck - Pipe / Fittings","General Appearance","Equipment Related","","","","","Will be done concurrently with P crane job ballast passge voy 29","2019-02-13","","Completed","2019-02-04","No","No","No","Internal"]
[null,null,null,null,3303,"23_2019-09-20 14:54:20.000","2019-01-13","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Old scrap to remove during the garbage landings and all the big and heavy items at Yiulian","Miscellaneous","General Appearance","Equipment Related","","","","","Will be done at singapore west bound Voy 29","2019-02-13","","Completed","2019-02-13","No","No","No","Internal"]
[null,null,null,null,3306,"23_2019-09-23 14:54:20.000","2019-01-13","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Access door for front windows of the bridge, hinge broken ","Accommodation","General Appearance","Equipment Related","","","","","Completed","2019-02-13","","Completed","2019-02-18","No","No","No","Internal"]
[null,null,null,null,3307,"23_2019-09-24 14:54:20.000","2019-01-13","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Few cable supports around accommodation wasted to renew","Accommodation","General Appearance","Equipment Related","","","","","Completed","2019-02-13","","Completed","2019-02-22","No","No","No","Internal"]
[null,null,null,null,3318,"23_2019-08-05 14:54:19.999","2019-01-13","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Emer gen air intake flap support plate on top corroded and holed","E/R - Aux. Engine","General Appearance","Equipment Related","","","","","Same has been repaired","2019-02-13","","Completed","2019-02-22","No","No","No","Internal"]
[null,null,null,null,3352,"23_2019-07-08 14:54:19.995","2019-01-14","Defect","Ship Staff","Ship Staff Insp.","ME viscotherm valve not holding. Need to replace valve for maintenance on viscotherm seal","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Valve renewed.","2019-04-30","DHAW190006","Completed","2019-03-20","No","No","No","Internal"]
[null,null,null,null,3377,"23_2019-06-03 14:54:19.995","2019-01-15","Defect","Ship Staff","Ship Staff Insp.","HFO FO Settling tank level gauge not operational","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Awaiting for supply.","2019-06-30","DHAW190034","Completed","2019-06-28","No","No","No","Internal"]
[null,null,null,null,9370,"23_Thu Jan 02 2020 11:53:39 GMT+0000","2019-01-24","Observation","Owner / Marine / Tech. Suptd.","Nav Audit / Verification","The forward anchor light (low) was not working at the time of the inspection.","Navigation - Others","Navigation","Equipment Related","","","","","","2019-01-30","","Completed","2019-01-22","No","No","No","Internal","light repaired and replacement spare arranged"]
[null,null,null,null,9371,"23_Thu Jan 02 2020 11:55:46 GMT+0000","2019-01-24","Observation","Owner / Marine / Tech. Suptd.","Nav Audit / Verification","The training imparted to deck officers with regards to GMDSS equipment was not recorded in the GMDSS log book.","Navigation - GMDSS & Communication","Navigation","Knowledge Based","4.21","High","","","Training being recorded in GMDSS Log Book.","2019-01-30","","Completed","2019-01-27","No","No","No","Internal"]
[null,null,null,null,9372,"23_Thu Jan 02 2020 11:57:34 GMT+0000","2019-01-24","Non Conformity","Owner / Marine / Tech. Suptd.","Nav Audit / Verification","The Master's Standing orders not signed by the A/Bs forming part of the Nav. watches at sea.","Navigation - Others","Navigation","Human Error","4.1","High","","","Master's  Standing Orders were read & signed by all Watch keeping Ratings. ","2019-01-30","","Completed","2019-01-25","No","No","No","Internal"]
[null,null,null,null,3297,"23_2019-09-14 14:54:20.000","2019-01-26","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Stripping pump discharge pressure gauge at CCR & P/RM not responding.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","line to discharge pressure gauge purged with air. Tested &  found to be working satisfactory.","2019-02-13","","Completed","2019-02-04","No","No","No","Internal"]
[null,null,null,null,3302,"23_2019-09-19 14:54:20.000","2019-01-26","Defect","Ship Staff","Ship Staff Insp.","Excess Gas Control valve hunting","Inert Gas","General Appearance","Equipment Related","","","","","Service requested for shore technician","2019-02-15","DHAW190045","Completed","2019-02-13","No","No","No","Internal"]
[null,null,null,null,3319,"23_2019-08-06 14:54:19.999","2019-01-26","Defect","Ship Staff","Ship Staff Insp.","#5 Unit ME fuel pump cut off air solenoid getting stuck","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Solenoid valve overhauled.All parts cleaned and lubricated.","2019-02-15","","Completed","2019-02-08","No","No","No","Internal"]
[null,null,null,null,9939,"23_20/01/2020 5:35:57 PM","2019-01-28","Non Conformity","Ship Staff","Ship Staff Insp.","Use of wrong form  for updating monthly KPI  data. Form no 05 05 00 001 00 was used instead of 05.05.00.001.01","Documentation","Cert. & Docu.","Human Error","5.8","Medium","","","Corrected.","2019-02-28","","Completed","2019-02-22","No","No","No","Internal"]
[null,null,null,null,3353,"23_2019-07-09 14:54:19.995","2019-01-29","Defect","Ship Staff","Ship Staff Insp.","#1 AE TC/Engine rpm meter erratic ","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Gauge needle adjusted.","2019-04-30","DHAW190043","Completed","2019-03-20","No","No","No","Internal"]
[null,null,null,null,3381,"23_2019-06-07 14:54:19.995","2019-01-29","Defect","Ship Staff","Ship Staff Insp.","No.1 SW Serv pump leaking from mechanical seal","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Mechanical seal replaced in yard.","2019-06-15","DHAW190051","Completed","2019-06-18","No","No","No","Internal"]
[null,null,null,null,3301,"23_2019-09-18 14:54:20.000","2019-02-01","Defect","Ship Staff","Ship Staff Insp.","STBD SIDE GANGWAY AIR PIPE CONNECTION TO AIR MOTOR WASTED.","Deck - Pipe / Fittings","General Appearance","Equipment Related","","","","","Completed","2019-02-05","","Completed","2019-02-02","No","No","No","Internal"]
[null,null,null,null,3300,"23_2019-09-17 14:54:20.000","2019-02-03","Defect","Ship Staff","Ship Staff Insp.","Deck seal drain pipe hole in the welding seam.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","IGS PUMP STOPPED. DECK SEAL WATER DRAINED.DRAIN PIPE OVERHAULED & REPAIRED IN E/RM WORKSHOP.","2019-02-10","","Completed","2019-02-04","No","No","No","Internal"]
[null,null,null,null,3308,"23_2019-09-25 14:54:20.000","2019-02-03","Defect","Ship Staff","Ship Staff Insp.","Aft air horn handle holding clip on Stbd bridge wing wasted.","Accommodation","General Appearance","Equipment Related","","","","","Completed","2019-02-20","","Completed","2019-02-18","No","No","No","Internal"]
[null,null,null,null,3305,"23_2019-09-22 14:54:20.000","2019-02-05","Defect","Ship Staff","Ship Staff Insp.","Gas equipments found to be showing faulty readings & consuming battery after 2-3 times of equipment use only.","Miscellaneous","General Appearance","Equipment Related","","","","","equipments calibrated. Problem persists. Equipmets, batteries replaced . Found to be working good.","2019-02-14","","Completed","2019-02-13","No","No","No","Internal"]
[null,null,null,null,3317,"23_2019-08-04 14:54:19.999","2019-02-07","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Stbd vecs trasmiter box nut bolts rusted and broken","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","broken bolt & nut replaced. Box secured.","2019-03-07","","Completed","2019-02-26","No","No","No","Internal"]
[null,null,null,null,3321,"23_2019-08-08 14:54:19.999","2019-02-07","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Port manifold gratings rusted","Miscellaneous","General Appearance","Equipment Related","","","","","Port side manifold grating dismantled, hydroblasted & painted.","2019-03-07","","Completed","2019-03-02","No","No","No","Internal"]
[null,null,null,null,3327,"23_2019-08-14 14:54:19.995","2019-02-07","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","\"C\" deck acc. Doors unable to lock from inside","Accommodation","General Appearance","Equipment Related","","","","","lubrication & freeing of locking arrangement carried out. Locking arrangement moving freely now.","2019-03-07","","Completed","2019-03-07","No","No","No","Internal"]
[null,null,null,null,3334,"23_2019-08-21 14:54:19.995","2019-02-12","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","port side hose handling crane oil leaking","Deck - Machinery","General Appearance","Equipment Related","","","","","Counter-Balance block Dowty Seal Ring renewed","2019-05-15","","Completed","2019-03-08","No","No","No","Internal"]
[null,null,null,null,3378,"23_2019-06-04 14:54:19.995","2019-02-12","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","E/R sludge to slop transfer line section in upper deck shows signs of corrosion","Deck - Pipe / Fittings","General Appearance","Equipment Related","","","","","Job carried out in dry dock","2019-06-25","","Completed","2019-06-20","No","No","No","Internal"]
[null,null,null,null,3320,"23_2019-08-07 14:54:19.999","2019-02-12","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Hydroblaster discharge line damaged sections to renew","Deck - Machinery","General Appearance","Equipment Related","","","","","Damaged section renewed with spare available onboard.","2019-04-30","","Completed","2019-02-25","No","No","No","Internal"]
[null,null,null,null,3322,"23_2019-08-09 14:54:19.999","2019-02-12","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Stbd side A deck scrupper drain line flange gasket to renew","Deck - Pipe / Fittings","General Appearance","Equipment Related","","","","","fault finding carried out in the flange by inserting fire hose in the drain on A & C deck stbd side respectively. Fire pump started, water passed with pressure no leak in the flanges found from c to upper deck.","2019-03-28","","Completed","2019-03-05","No","No","No","Internal"]
[null,null,null,null,3379,"23_2019-06-05 14:54:19.995","2019-02-13","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","No.2 D/G Control Air Reducer top cover flange with soft patch.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Gasket renewed & repair work carried out in Drydock","2019-06-28","","Completed","2019-06-20","No","No","No","Internal"]
[null,null,null,null,3299,"23_2019-09-16 14:54:20.000","2019-02-13","Defect","Ship Staff","Ship Staff Insp.","STbd. anchor chain stopper tongue jammed.","Deck - Pipe / Fittings","General Appearance","Equipment Related","","","","","Freeing of anchor chain stopper tongue carried out. Lubrication carried out.","2019-02-20","","Completed","2019-02-13","No","No","No","Internal"]
[null,null,null,null,3332,"23_2019-08-19 14:54:19.995","2019-02-23","Defect","Ship Staff","Ship Staff Insp.","In pumproom guide wire attached to heaving line of neil robertson stretcher corroded & broken.","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","Guide wire replaced with new one. Coat of grease in place.","2019-02-25","","Completed","2019-02-25","No","No","No","Internal"]
[null,null,null,null,3315,"23_2019-08-02 14:54:19.999","2019-02-24","Defect","Ship Staff","Ship Staff Insp.","COT Slop STBD. IG leak from tank dome.","Deck - Pipe / Fittings","General Appearance","Equipment Related","","","","","SLOP STBD IG v/v shut, COT depressurized, Rubber packing renewed, Leak test carried out with soap solution, No leak sound observed.","2019-02-25","","Completed","2019-02-24","No","No","No","Internal"]
[null,null,null,null,9940,"23_20/01/2020 6:25:24 PM","2019-02-25","Non Conformity","Ship Staff","Ship Staff Insp.","Obsolete SSAS  switch not clearly marked .The old Jrc SSAS Switch on board wascnot labelled as not in use leading to confusion while testing the SSAS.  ","Navigation - GMDSS & Communication","ISPS Related","Human Error","7.4","Low","","","Labeling done.","2019-03-01","","Completed","2019-02-25","No","No","No","Internal"]
[null,null,null,null,3316,"23_2019-08-03 14:54:19.999","2019-02-25","Defect","Ship Staff","Ship Staff Insp.","Crack on top plate observed  in ODME hydraulic v/v  to slop (S) COV 511","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","Plate dismantled & repaired by grooving in E/rm workshop.","2019-02-26","","Completed","2019-02-25","No","No","No","Internal"]
[null,null,null,null,3325,"23_2019-08-12 14:54:19.995","2019-02-25","Defect","Ship Staff","Ship Staff Insp.","FWD. mooring winch drum no W1/1 brake tightening limit indicator pin got cracked during greasing & lubrication.","Deck - Pipe / Fittings","General Appearance","Equipment Related","","","","","pin dismantled & hot work repair carried out in E/rm workshop.","2019-02-28","","Completed","2019-03-02","No","No","No","Internal"]
[null,null,null,null,3326,"23_2019-08-13 14:54:19.995","2019-02-26","Defect","Ship Staff","Ship Staff Insp.","Port side life raft one craddle leg deformed.","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","Life raft removed from stowed position. New craddle fabricated in e/rm workshop & fit back in position.","2019-03-09","","Completed","2019-03-09","No","No","No","Internal"]
[null,null,null,null,3328,"23_2019-08-15 14:54:19.995","2019-02-27","Defect","Ship Staff","Ship Staff Insp.","slings found broken, deterioted condition on 06 forward mooring drums. Sling is used to connect mooring wire eye to a rigid point in drum.","Deck - Machinery","General Appearance","Equipment Related","","","","","one by one all  06 mooring wires transferrred to other drums. Then broken slings removed. New slings in place. Coat of grease applied on newly fitted slings. All 06 mooring wires shifted back to their respective drums.","2019-03-15","","Completed","2019-03-08","No","No","No","Internal"]
[null,null,null,null,9941,"23_20/01/2020 5:39:05 PM","2019-02-28","Defect","Ship Staff","Ship Staff Insp.","life raft cradle stand support broken due to vessels rolling and pitching.","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.28","Very High","","","Rectified.","2019-02-28","","Completed","2019-03-07","No","No","No","Internal"]
[null,null,null,null,3335,"23_2019-08-22 14:54:19.995","2019-03-01","Defect","Ship Staff","Ship Staff Insp.","Aux Boiler # 1 heating coils leaking","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","3nos of heating coil found leaking and repaired by welding. Pressure Tested and found ok.","2019-03-20","","Completed","2019-03-12","No","No","No","Internal"]
[null,null,null,null,3354,"23_2019-07-10 14:54:19.995","2019-03-01","Defect","Ship Staff","Ship Staff Insp.","Aux Boiler # 1 atomising steam stop valve leaking","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","Valve renewed.","2019-03-25","","Completed","2019-03-19","No","No","No","Internal"]
[null,null,null,null,3355,"23_2019-07-11 14:54:19.995","2019-03-01","Defect","Ship Staff","Ship Staff Insp.","Aux Boiler # 2 level rising when on stby.Suction valve to EGB Circulating Pump  suspected leaking.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","Boiler Circulating Water Pump suction valve seat lapped.","2019-03-30","","Completed","2019-03-19","No","No","No","Internal"]
[null,null,null,null,3324,"23_2019-08-11 14:54:19.995","2019-03-01","Defect","Ship Staff","Ship Staff Insp.","During routine inspection it was found that water is leaking to rotory pump gear oil box of hydroblasting machine.","Miscellaneous","General Appearance","Equipment Related","","","","","rotory pump overhauled, broken o - ring replaced. Gear oil renewed. Hydro blasting machine tested working good.","2019-03-05","","Completed","2019-03-04","No","No","No","Internal"]
[null,null,null,null,3323,"23_2019-08-10 14:54:19.995","2019-03-02","Defect","Ship Staff","Ship Staff Insp.","During weekly boat drill, it was found that the life boat rudder is not responding during applying steering movement. Steering was also moving free.","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","during fault finding it was found that the pully which carries wire for steering movement & connected to rudder is having nut which is partiallly damage. Arrangement has been made for the nut and steering is working good.","2019-03-04","","Completed","2019-03-04","No","No","No","Internal"]
[null,null,null,null,3329,"23_2019-08-16 14:54:19.995","2019-03-04","Defect","Ship Staff","Ship Staff Insp.","hospital weather proof door found jammed. Galley entrance fire door jammed. 'A' deck stbd side fire door jammed.","Accommodation","General Appearance","Equipment Related","","","","","doors repaied, hinges tightened, locking arrangement lubricated & freed. All doors opening, closing & locking freely after repair.","2019-03-09","","Completed","2019-03-08","No","No","No","Internal"]
[null,null,null,null,3330,"23_2019-08-17 14:54:19.995","2019-03-04","Defect","Ship Staff","Ship Staff Insp.","Deck & engine changing room not provided with hydraulic door closer. Doos found banging on bulkheads when vessel was moderately rolling.","Accommodation","General Appearance","Equipment Related","","","","","Hydraulic door closer fitted on doors.","2019-03-09","","Completed","2019-03-06","No","No","No","Internal"]
[null,null,null,null,3385,"23_2019-10-03 05:59:28.000","2019-03-05","Defect","Ship Staff","Ship Staff Insp.","Cracks on various portholes found Galley - 04 portholes, 3/E cabin - 01 port hole","Accommodation","General Appearance","Equipment Related","","","","","Portholes received , same to be fixed","2019-07-28","","Completed","2019-07-25","No","No","No","Internal"]
[null,null,null,null,3331,"23_2019-08-18 14:54:19.995","2019-03-06","Defect","Ship Staff","Ship Staff Insp.","one galley A/C vent grills found broken & missing.","Accommodation","General Appearance","Equipment Related","","","","","A/C vent grill dismantled. Tag wielded grills & fitted back in place.","2019-03-11","","Completed","2019-03-11","No","No","No","Internal"]
[null,null,null,null,3336,"23_2019-08-23 14:54:19.995","2019-03-07","Defect","Ship Staff","Ship Staff Insp.","Upper deck alley, Deck & engine changing locker floor found in rusted condition.","Accommodation","General Appearance","Equipment Related","","","","","upper deck alley bulkhead painted white. Upper deck alley, deck, engine changing locker floor derusted & painted green.","2019-03-14","","Completed","2019-03-13","No","No","No","Internal"]
[null,null,null,null,3344,"23_2019-08-31 14:54:19.995","2019-03-12","Defect","Ship Staff","Ship Staff Insp.","one gangway pneumatic motor not operational.","Deck - Machinery","General Appearance","Equipment Related","","","","","motor overhauled & repaired. Working satisfactory.","2019-03-16","","Completed","2019-03-14","No","No","No","Internal"]
[null,null,null,null,3356,"23_2019-07-12 14:54:19.995","2019-03-13","Defect","Ship Staff","Ship Staff Insp.","Aux Boiler # 2 Port side blowdown valve choked. To clear.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","Both blow-down valves removed, cleared and put back.","2019-04-15","","Completed","2019-03-19","No","No","No","Internal"]
[null,null,null,null,3363,"23_2019-07-19 14:54:19.995","2019-03-13","Defect","Ship Staff","Ship Staff Insp.","NO.1 MAIN AB FEED PUMP SHAFT TO RENEW WITH NEW ORIGINAL SPARE.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","Overhauling, shaft assembly with new original spare - completed.","2019-04-20","","Completed","2019-04-22","No","No","No","Internal"]
[null,null,null,null,3365,"23_2019-07-21 14:54:19.995","2019-03-13","Defect","Ship Staff","Ship Staff Insp.","HOTWELL OBSERVATION TANK PORT SIGHTGLASS TO RENEW.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","Spares received. Planned to do job during Yard Repairs.","2019-05-01","DHAW190115","Completed","2019-05-27","No","No","No","Internal"]
[null,null,null,null,3382,"23_2019-06-08 14:54:19.995","2019-03-13","Defect","Ship Staff","Ship Staff Insp.","Emergency Fire Pump Volute Cover damaged iwo gland packing well. ","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","spare received.","2019-06-15","DHAW190075","Completed","2019-07-04","No","No","No","Internal"]
[null,null,null,null,3338,"23_2019-08-25 14:54:19.995","2019-03-14","Defect","Ship Staff","Ship Staff Insp.","ODME valve to slop (S) COV 513 found hydraulic oil leaking into the valve & over flowed on deck.","Deck - Pipe / Fittings","General Appearance","Equipment Related","","","","","valve hydraulic line isolated. Valve drain plug opened & hydraulic oil drained.leaking side part overhauled & found rubber seal was new but fit in wrong way. Fit in a correct way & box back. Valve operated & found no leaks in the valve.","2019-03-15","","Completed","2019-03-14","No","No","No","Internal"]
[null,null,null,null,3339,"23_2019-08-26 14:54:19.995","2019-03-14","Defect","Ship Staff","Ship Staff Insp.","Fire doors to Galley in front of ship's office, fire door on A deck stbd side not closing properly.","Accommodation","General Appearance","Equipment Related","","","","","Base of the door frame obstructing door to close smoothly. Suspected obstructed steel part hammered. Door is opening 7 closing smoothly.","2019-03-16","","Completed","2019-03-15","No","No","No","Internal"]
[null,null,null,null,3340,"23_2019-08-27 14:54:19.995","2019-03-14","Defect","Ship Staff","Ship Staff Insp.","during port side hose handling crane trial prior arrival load port Angra Dos Reis, Brazil it was found oil is leaking from a block connected to a cylinder. Other cylinder block which was repaired was found intact.","Deck - Machinery","General Appearance","Equipment Related","","","","","over hauled, copper seal fabrication in progress.","2019-04-18","","Completed","2019-03-17","No","No","No","Internal"]
[null,null,null,null,3341,"23_2019-08-28 14:54:19.995","2019-03-14","Defect","Ship Staff","Ship Staff Insp.","during trial of mooring winches prior arrival Angra Dos Reis, Brazil it was found that Forward spring line operating lever found jammed. ","Deck - Machinery","General Appearance","Equipment Related","","","","","Hydraulic inlet, return & drain line to winch isolated, lever & block buffed paint removed, lever with block removed & rectification in E/rm workshop in progress.","2019-03-18","","Completed","2019-03-15","No","No","No","Internal"]
[null,null,null,null,3362,"23_2019-07-18 14:54:19.995","2019-03-14","Defect","Ship Staff","Ship Staff Insp.","No.2 SW Service Pump El Motor Burnt.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","New EL Motor received, and installed.","2019-04-20","DHAW190073","Completed","2019-05-01","No","No","No","Internal"]
[null,null,null,null,3343,"23_2019-08-30 14:54:19.995","2019-03-15","Defect","Ship Staff","Ship Staff Insp.","Shackles on davit near p/rm, ig isolation v/v platform, manifold area, poop deck area, foc'le area found jammed & wasted.","Deck - Pipe / Fittings","General Appearance","Equipment Related","","","","","shacked derusted, freed, replaced with new one.","2019-03-18","","Completed","2019-03-17","No","No","No","Internal"]
[null,null,null,null,3342,"23_2019-08-29 14:54:19.995","2019-03-17","Defect","Ship Staff","Ship Staff Insp.","U - clamp found broken on steam return line to slop stbd.","Deck - Pipe / Fittings","General Appearance","Equipment Related","","","","","replaced with new one.","2019-03-18","","Completed","2019-03-18","No","No","No","Internal"]
[null,null,null,null,3345,"23_2019-07-01 14:54:19.999","2019-03-17","Defect","Ship Staff","Ship Staff Insp.","chain hooks on catwalk, L/B area, foam monitor area, Provision gantry area, bridge wing area, suez canal light post area found jammed, frozen.","Deck - Pipe / Fittings","General Appearance","Equipment Related","","","","","Lubricated, freed & replaced as required.","2019-03-22","","Completed","2019-03-20","No","No","No","Internal"]
[null,null,null,null,3346,"23_2019-07-02 14:54:19.995","2019-03-18","Defect","Ship Staff","Ship Staff Insp.","drain pipe on funnel deck, d deck Port & stbd side found jammed.","Accommodation","General Appearance","Equipment Related","","","","","air blown through, passage cleared.","2019-03-21","","Completed","2019-03-21","No","No","No","Internal"]
[null,null,null,null,3348,"23_2019-07-04 14:54:19.995","2019-03-19","Defect","Ship Staff","Ship Staff Insp.","hole found in port side capstan pneumatic pipe ","Deck - Pipe / Fittings","General Appearance","Equipment Related","","","","","Hole sealed with compund. Followed by painting.","2019-03-22","","Completed","2019-03-22","No","No","No","Internal"]
[null,null,null,null,3349,"23_2019-07-05 14:54:19.995","2019-03-19","Defect","Ship Staff","Ship Staff Insp.","operating lever of stbd side capstan found jammed","Deck - Pipe / Fittings","General Appearance","Equipment Related","","","","","lever freed, lubricated.","2019-03-22","","Completed","2019-03-22","No","No","No","Internal"]
[null,null,null,null,3347,"23_2019-07-03 14:54:19.995","2019-03-21","Defect","Ship Staff","Ship Staff Insp.","Port side SOPEP wielden pump not working.","Deck - Pipe / Fittings","General Appearance","Equipment Related","","","","","wielden pump overhauled piston found jammed. Freed, lubricated the piston.","2019-03-21","","Completed","2019-03-21","No","No","No","Internal"]
[null,null,null,null,3383,"23_2019-10-01 05:59:28.000","2019-03-27","Defect","Ship Staff","Ship Staff Insp.","Bridge Split type A/C having low insulation.","Miscellaneous","General Appearance","Equipment Related","","","","","RENEWED AT DRY DOCK","2019-06-05","DHAW190127","Completed","2019-06-10","No","No","No","Internal"]
[null,null,null,null,3359,"23_2019-07-15 14:54:19.995","2019-04-03","Defect","Ship Staff","Ship Staff Insp.","Accomodation Emc'y exit fire doors at D, C deck found at end parts.","Accommodation","General Appearance","Equipment Related","","","","","caps Filled with devcon. Followed by 3 primer coats + final white coat.","2019-04-06","","Completed","2019-04-06","No","No","No","Internal"]
[null,null,null,null,3350,"23_2019-07-06 14:54:19.995","2019-04-05","Defect","Ship Staff","Ship Staff Insp.","WBT FPT Manhole rubber gasket found damaged during 6 monthly inspection.","Deck - Pipe / Fittings","General Appearance","Equipment Related","","","","","replaced with new rubber gasket.","2019-05-07","","Completed","2019-04-05","No","No","No","Internal"]
[null,null,null,null,3358,"23_2019-07-14 14:54:19.995","2019-04-05","Defect","Ship Staff","Ship Staff Insp.","belling arrangement in the bell for navigational fog signal at forecastle deck found broken.","Deck - Pipe / Fittings","General Appearance","Equipment Related","","","","","Belling arrangement rectify 7 found to be in order.","2019-04-07","","Completed","2019-04-06","No","No","No","Internal"]
[null,null,null,null,3360,"23_2019-07-16 14:54:19.995","2019-04-05","Defect","Ship Staff","Ship Staff Insp.","port & stbd side life boat platforms found corroded, wasted, broken.","Deck - Pipe / Fittings","General Appearance","Equipment Related","","","","","renewed with new one","2019-04-25","","Completed","2019-04-25","No","No","No","Internal"]
[null,null,null,null,9942,"23_20/01/2020 6:28:32 PM","2019-04-25","Non Conformity","Ship Staff","Ship Staff Insp.","Engine room Dead Man alarm Activation key not found in place. The Key was Found to be lying on the floor nearby/ it was immediately placed in the proper postition.","Miscellaneous","Eng. / Strg. Comp.","Human Error","10.4","High","","","Activation key was immediately placed in the proper postition.","2019-04-29","","Completed","2019-04-25","No","No","No","Internal"]
[null,null,null,null,9943,"23_20/01/2020 5:14:16 PM","2019-05-11","Non Conformity","Class Surveyor","ISM Audit","S1.Noted from M/E NOx technical file, C/E stated this number was mis-entered by mistaken, and replaced nozzles are exactly same as the original. The company may wish to take some preventative actions to avoid similar issues lead to a non-conformance in future.","Documentation","Cert. & Docu.","Human Error","10.5","Low","","","After confirming with the actual spare parts record that the used parts were having the genuine stamp from maker, the entries were corrected in presence of the LR surveyor countersigned by current 2/eng and Chief engineer","2019-08-10","","Completed","2019-09-18","No","No","No","External"]
[null,null,null,null,9944,"23_20/01/2020 5:17:11 PM","2019-05-11","Non Conformity","Class Surveyor","ISM Audit","Noted in requisition request record that a number of previous requests made in 2017 & 2018 are still pending. The crews stated that all these requests have already closed, and record should have been updated. The company may wish to take some preventative actions to avoid similar issues leading to a non-conformance in future.\n\n","Miscellaneous","Communication","External Factors","","","","","Arranged with Procure department to clear the pending PO since the goods have been received and vessel presently had no access anymore to the pertaining POs as workflow has been forwarded to procure. Purchase department confirmed on 06 Aug 29019 that same cleared from their side and the issue is resolved. IT department corrected the replication issue with PAL and requisition status showed same on ship and in office . ","2019-08-10","","Completed","2019-09-18","No","No","No","External"]
[null,null,null,null,3441,"23_2019-05-17 14:54:19.995","2019-05-13","Defect","Ship Staff","Ship Staff Insp.","Rudder Sea Water Cooling overhaed pipe leaking. No intermediate stop valve provided.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Intermediate valve installed. Temporary arrangement made, permenent line to be renewed later.","2019-08-31","","Completed","2019-08-31","No","No","No","Internal"]
[null,null,null,null,9945,"23_20/01/2020 5:28:06 PM","2019-05-13","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Stbd Side navigation light was found fused during the course of the inspection.","Navigation - Others","Navigation","Equipment Related","4.8","Medium","","","Navigation light was changed on same day.","2019-05-31","","Completed","2019-05-13","No","No","No","Internal"]
[null,null,null,null,9948,"23_20/01/2020 5:31:01 PM","2019-05-13","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Pre-departure & pre-arrival test checks entries were missed out in the deck logbook for this port Tianjin.","Navigation - Others","Navigation","Human Error","4.3","Medium","","","Missed entries inserted as required.","2019-05-31","","Completed","2019-05-14","No","No","No","Internal"]
[null,null,null,null,3473,"23_2019-07-28 14:54:19.995","2019-05-18","Defect","Ship Staff","Ship Staff Insp.","ODME stripping line flowmeter malfunctioning.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","Shore servicing","2019-06-15","","Completed","2019-06-06","No","No","No","Internal"]
[null,null,null,null,9946,"23_20/01/2020 6:31:16 PM","2019-05-22","Non Conformity","Ship Staff","Ship Staff Insp.","Port side lifeboat air hose pressure gauge found faulty. Requisition raised and will change as soon as received.","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.28","Very High","","","Pressure guage replaced.","2019-06-10","","Completed","2019-06-15","No","No","No","Internal"]
[null,null,null,null,3469,"23_2019-04-14 14:54:19.995","2019-06-25","Defect","Ship Staff","Ship Staff Insp.","WALKWAY RAMP IN BREAK OF ACCOMMODATION PORT SIDE DOES NOT HAVE RAILING, BY DESIGN,  TO SUPPORT THE PERSON WALKING ","Miscellaneous","General Appearance","Equipment Related","","","","","Railing fabricated and Fixed using cold work by bracket and bolt ","2019-09-25","","Completed","2019-09-30","No","No","No","Internal"]
[null,null,null,null,3372,"23_2019-07-29 14:54:19.995","2019-06-27","Defect","Ship Staff","Ship Staff Insp.","KINK IN STBD ANCHOR","Deck - Machinery","General Appearance","Equipment Related","","","","","COMPLETED","2019-07-20","","Completed","2019-07-23","No","No","No","Internal"]
[null,null,null,null,3388,"23_2019-10-06 05:59:28.000","2019-06-27","Defect","Ship Staff","Ship Staff Insp.","VALVE REMOTE CONTROL  SYSTEM HYDRAULIC PRESSURE ALARM SETTING TO BE CORRECTED ","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","Alarm setting Corrected and working fine","2019-08-03","","Completed","2019-08-03","No","No","No","Internal"]
[null,null,null,null,3389,"23_2019-10-07 05:59:28.000","2019-06-27","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","BILGES TANK TOP TO MAKE DRY OFF WATER AND PAINT","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","WATER DRIED AND PAINTED","2019-08-27","","Completed","2019-07-08","No","No","No","Internal"]
[null,null,null,null,9947,"23_20/01/2020 6:34:46 PM","2019-06-30","Defect","Ship Staff","Ship Staff Insp.","During singapore pre arrival checks it was found that pilot ladder split pieces are broken at few places and some of them were fabricated onboard.","Deck - Machinery","ISM Related","Equipment Related","5.47","Medium","","","Broken split pieces were renewed onboard and requisitin raised for the new pilot ladder","2019-07-15","","Completed","2019-07-04","No","No","No","Internal"]
[null,null,null,null,3437,"23_2019-05-13 14:54:19.995","2019-07-01","Defect","Ship Staff","Ship Staff Insp.","MSB unit cooler S.W.pipe line clogging/less water flow","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Pipe lines to be replaced with PVC pipelines","2019-09-15","","Completed","2019-08-22","No","No","No","Internal"]
[null,null,null,null,6702,"23_21/11/2019 3:25:50 AM","2019-07-02","Defect","Ship Staff","Ship Staff Insp.","Doppler log screen gets frozen. Display was replaced but the issue is still there.","Navigation - Echo Sounder / Speed Log","Navigation","Equipment Related","4.7","High","","","Furuno technician attended vessel on 04 July 2019, and replaced the fuse and found Doppler operational, after few hours the screen again froze. As per Furuno technician’s recommendation the LCD display unit was ordered and replaced by ETO on board. After a week of operation the same issue was repeating. \n\n\n\nFuruno technician attended at Singapore, working satisfactory.","2020-01-30","","Completed","2020-02-07","No","No","No","Internal","follow up serv with the makers will be arranged at next port of call."]
[null,null,null,null,3686,"23_15/10/2019 6:10:51 AM","2019-07-03","Defect","Ship Staff","Ship Staff Insp.","Monorail crane electric cable automatic winding not working, same has to be winded by a person standing on top","Deck - Machinery","Cargo / Ballast Systems","Equipment Related","8.5","Very High","","","Electrical cable is renewed and automatic winding investigation in progress.","2019-10-30","","Completed","2019-12-04","No","No","No","Internal"]
[null,null,null,null,3386,"23_2019-10-04 05:59:28.000","2019-07-04","Defect","Ship Staff","Ship Staff Insp.","EGB Steam Outlet Header tubes leaking ","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","Emergency repair work carried out by Shore workshop at singapore,permanent reapir work will be carried out at Map-Ta-phut","2019-08-09","DHAW195086","Completed","2019-08-15","No","No","No","Internal"]
[null,null,null,null,3390,"23_2019-10-08 05:59:28.000","2019-07-04","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","LAGGING OF BOILER BLOW DOWN OVERBOARD VALVE TO REPLACE","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","RENEWED THE LAGGING","2019-07-11","","Completed","2019-07-09","No","No","No","Internal"]
[null,null,null,null,3391,"23_2019-10-09 05:59:28.000","2019-07-04","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","1 S F.O.TANK HEATING LINE LEAKAGE TO RECTIFY AND LAGGING TO REPLACE","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","LEAK RECTIFIED AND RENEWED THE LAGGING","2019-07-11","","Completed","2019-07-08","No","No","No","Internal"]
[null,null,null,null,3392,"23_2019-10-10 05:59:28.000","2019-07-04","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ECONOMISER FEED WATER PUMP SAVE ALL TRAY TO CLEAN","Miscellaneous","General Appearance","Equipment Related","","","","","CLEANED AND PAINTED","2019-07-11","","Completed","2019-07-10","No","No","No","Internal"]
[null,null,null,null,3393,"23_2019-10-11 05:59:28.000","2019-07-04","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ICO LUBE UNIT CYLINDER OIL PLUG LEAKING, TO RECTIFY","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","LEAK RECTIFIED","2019-07-11","","Completed","2019-07-10","No","No","No","Internal"]
[null,null,null,null,3394,"23_2019-10-12 05:59:28.000","2019-07-04","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","AUX BOILER FO SUPPLY PUMP SAVE ALL TO CLEAN","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","SAVED ALL TO CLEAN","2019-07-11","","Completed","2019-07-11","No","No","No","Internal"]
[null,null,null,null,3395,"23_2019-10-13 05:59:28.000","2019-07-04","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","WORKSHOP TO ARRANGE","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","WORKSHOP ARRANGED","2019-07-14","","Completed","2019-07-13","No","No","No","Internal"]
[null,null,null,null,3396,"23_2019-10-16 05:59:28.000","2019-07-04","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","STUFFING BOX DRAIN TANK SAVE ALL TO CLEAN","Miscellaneous","General Appearance","Equipment Related","","","","","CLEANED","2019-07-14","","Completed","2019-07-08","No","No","No","Internal"]
[null,null,null,null,3397,"23_2019-10-17 05:59:28.000","2019-07-04","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","L.O.COOLER INLET VALVE LEAK TO RECTIFY AND AREA TO CLEAN","Miscellaneous","General Appearance","Equipment Related","","","","","RECTIFIED THE LEAK","2019-08-03","","Completed","2019-08-01","No","No","No","Internal"]
[null,null,null,null,3398,"23_2019-10-18 05:59:28.000","2019-07-04","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","STUFFING BOX DRAIN TANK SAVE ALL TO CLEAN","Miscellaneous","General Appearance","Equipment Related","","","","","RENEWED THE LAGGING","2019-07-14","","Completed","2019-08-24","No","No","No","Internal"]
[null,null,null,null,3399,"23_2019-10-19 05:59:28.000","2019-07-04","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","AIR CON ROOM LOOSE EQUIPMENT AND BOTTLE TO SECURE AND ARRANGE","Miscellaneous","General Appearance","Equipment Related","","","","","ARRANGED","2019-07-29","","Completed","2019-07-15","No","No","No","Internal"]
[null,null,null,null,3400,"23_2019-10-20 05:59:28.000","2019-07-04","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ONE OF THE AIRCON FAN  MOTOR TO INSTALL WITH BELT","Miscellaneous","General Appearance","Equipment Related","","","","","COMPLETED","2019-07-14","","Completed","2019-07-10","No","No","No","Internal"]
[null,null,null,null,3401,"23_2019-10-21 05:59:28.000","2019-07-04","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","LIGHT IN SOX SCRUBBER PUMP AREA TO MOUNT BACK ( AS LIGHT HAS BEEN REMOVED FOR INSTALLATION) AS AREA IS DARK","Elect. Mach. & Equip.","General Appearance","Equipment Related","","","","","COMPLETED","2019-08-03","","Completed","2019-08-10","No","No","No","Internal"]
[null,null,null,null,3402,"23_2019-10-22 05:59:28.000","2019-07-04","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","NEW LIGHT TO INSTALL NEAR ME,DG DAMPER AREA (NEWLY INSTALLED)","Elect. Mach. & Equip.","General Appearance","Equipment Related","","","","","COMPLETED","2019-09-03","","Completed","2019-08-10","No","No","No","Internal"]
[null,null,null,null,3403,"23_2019-06-09 14:54:19.999","2019-07-04","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","PACKING MATERIAL FOR EGCS SCRUBBER IS LYING ON DECK TO TRANSFER","Miscellaneous","General Appearance","Equipment Related","","","","","COMPLETED","2019-07-11","","Completed","2019-07-09","No","No","No","Internal"]
[null,null,null,null,3404,"23_2019-06-10 14:54:19.995","2019-07-04","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","NO.1 SW SERVICE PUMP LEAKING FROM SHAFT SEAL, TO RECTIFY","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","RECTIFIED","2019-08-03","","Completed","2019-07-26","No","No","No","Internal"]
[null,null,null,null,3405,"23_2019-06-11 14:54:19.995","2019-07-04","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","VARIOUS NEWLY INSTALLED PLATFORMS TO PAINT","Miscellaneous","General Appearance","Equipment Related","","","","","COMPLETED","2019-07-19","","Completed","2019-07-12","No","No","No","Internal"]
[null,null,null,null,3406,"23_2019-06-12 14:54:19.995","2019-07-04","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","VARIOUS NEWLY INSTALLED PIPE LINES TO PAINT","Miscellaneous","General Appearance","Equipment Related","","","","","COMPLETED","2019-07-19","","Completed","2019-07-12","No","No","No","Internal"]
[null,null,null,null,3407,"23_2019-06-13 14:54:19.995","2019-07-04","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ONE OF THE HYDROPHORE PUMP IS LEAKING FROM SHAFT, TO RECTFY","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","COMPLETED","2019-07-24","","Completed","2019-07-16","No","No","No","Internal"]
[null,null,null,null,3408,"23_2019-06-14 14:54:19.995","2019-07-04","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","FIRE ALARM CALL POINT BROKEN AT ENTRANCE FROM CHINA PASSAGE TO ENGINE ROOM TO REPLACE.","Elect. Mach. & Equip.","General Appearance","Equipment Related","","","","","COMPLETED","2019-08-04","","Completed","2019-07-13","No","No","No","Internal"]
[null,null,null,null,3409,"23_2019-06-15 14:54:19.995","2019-07-04","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","LAGGING MISSING FROM VARIOUS  BOILER MOUNTING, LIKE MAIN STEAM STOP VALVE, FEED WATER VALVE","Miscellaneous","General Appearance","Equipment Related","","","","","COMPLETED","2019-07-14","","Completed","2019-07-12","No","No","No","Internal"]
[null,null,null,null,3410,"23_2019-06-16 14:54:19.995","2019-07-04","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","MSB ROOM AIR CON IS NOT OPERATIONAL AS THE C.W.PIPE LINE IS CHOKED. LINES TO RENEW AS MATERIAL IS ALREADY ON BOARD.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","COMPLETED","2019-07-23","","Completed","2019-08-10","No","No","No","Internal"]
[null,null,null,null,3411,"23_2019-06-17 14:54:19.995","2019-07-04","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","IN FOAM ROOM VARIOUS PIPES, BOXES LYING UNSECURED TO REMOVE FROM THE AREA","Miscellaneous","General Appearance","Equipment Related","","","","","COMPLETED","2019-07-11","","Completed","2019-07-10","No","No","No","Internal"]
[null,null,null,null,3412,"23_2019-06-18 14:54:19.995","2019-07-04","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","PIPES AND METAL PLATES STILL LYING ON DECK TO TRANSFER O ITS DESIGNATED AREA","Miscellaneous","General Appearance","Equipment Related","","","","","COMPLETED","2019-07-11","","Completed","2019-07-10","No","No","No","Internal"]
[null,null,null,null,3413,"23_2019-06-19 14:54:19.995","2019-07-04","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","AT ENTRANCE OF PUMP ROOM IN FOAMBOX MANY UNWANTED ITEMS ARE KEPT TO CLEAR","Miscellaneous","General Appearance","Equipment Related","","","","","COMPLETED","2019-07-06","","Completed","2019-07-05","No","No","No","Internal"]
[null,null,null,null,3414,"23_2019-06-20 14:54:19.995","2019-07-04","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","PORTABLE FIRE EXTINGUISHER MISSING FROM THE BOX AT MID SHIP STORE ENTRANCE","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","COMPLETED","2019-07-06","","Completed","2019-07-05","No","No","No","Internal"]
[null,null,null,null,3415,"23_2019-06-21 14:54:19.995","2019-07-04","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","MIDSHIP STORE / SOPEP LOCKER IS FULL OF VARIOUS ITEMS FROM DOCKING, HENCE IT IS NOT ACCESSIBLE TO ARRANGE THE LOCKER.","Miscellaneous","General Appearance","Equipment Related","","","","","COMPLETED","2019-07-11","","Completed","2019-07-20","No","No","No","Internal"]
[null,null,null,null,3416,"23_2019-06-22 14:54:19.995","2019-07-04","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","THE GRATING OF PORT WINDLASS OPERATING AREA IS DAMAGED. TO RENEW.","Miscellaneous","General Appearance","Equipment Related","","","","","COMPLETED","2019-07-19","","Completed","2019-07-10","No","No","No","Internal"]
[null,null,null,null,3417,"23_2019-06-23 14:54:19.995","2019-07-04","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","SOME OF THE MOORING WIRE IS IN MUDY AND DRY CONDITION AFTER DOCKING. TO CLEAN AND GREASE","Miscellaneous","General Appearance","Equipment Related","","","","","ALL REPLACED WITH NEW ONES","2019-09-03","","Completed","2019-07-15","No","No","No","Internal"]
[null,null,null,null,3418,"23_2019-06-24 14:54:19.995","2019-07-04","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","D-DECK PORT SIDE AND C-DECK STBD SIDE DOOR NOT OPENING. TO RECTFY","Miscellaneous","General Appearance","Equipment Related","","","","","COMPLETED","2019-07-18","","Completed","2019-07-10","No","No","No","Internal"]
[null,null,null,null,3419,"23_2019-06-25 14:54:19.995","2019-07-04","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","WIND HIGH HIGH ALARM IS NOT OPERATIONAL. TO TROULE SHOOT AND RECTIFY","Elect. Mach. & Equip.","General Appearance","Equipment Related","","","","","COMPLETED","2019-07-19","","Completed","2019-07-25","No","No","No","Internal"]
[null,null,null,null,3420,"23_2019-06-26 14:54:19.995","2019-07-04","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","VALVE REMOTE CONTROL PUMP WHEN RUNNING, HIGH PRESSURE ALARM WAS PRESENT EVEN THOUGH PRESSURE WAS NORMAL. WHEN PUMP STARTED EVEN THOUGH PRESSURE IS HOLDING, LOW PRESSURE ALARM GETS ACTIVATED. TO TROUBLE SHOOT AND RECTIFY","Miscellaneous","General Appearance","Equipment Related","","","","","COMPLETED","2019-08-03","","Completed","2019-07-23","No","No","No","Internal"]
[null,null,null,null,3468,"23_2019-04-13 14:54:19.995","2019-07-04","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","THE COLOUR OF HELICOPTER AREA IS SAME AS DECK COLOR. IT SHOULD BE OF CONTRASTING COLOUR.","Miscellaneous","General Appearance","Equipment Related","","","","","Painting carried out with grey colour after derusting","2019-09-15","","Completed","2019-09-30","No","No","No","Internal"]
[null,null,null,null,3457,"23_2019-04-02 14:54:19.995","2019-07-05","Defect","Ship Staff","Ship Staff Insp.","STAYWIRE OF FWD MAST MISSING","Deck - Pipe / Fittings","General Appearance","Equipment Related","","","","","Awaiting good weather to carry out the job","2019-09-07","","Completed","2019-09-03","No","No","No","Internal"]
[null,null,null,null,3687,"23_15/10/2019 6:14:39 AM","2019-07-07","Defect","Ship Staff","Ship Staff Insp.","ME LO backwash filter diaphragm cracked and leaking","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","11.1","High","","","New valve fitted","2020-02-07","DHAW190214","Completed","2020-02-19","No","No","No","Internal","initial spares connected not suitable. spares arranged again for the next port of call in China"]
[null,null,null,null,3444,"23_2019-05-20 14:54:19.995","2019-07-08","Defect","Ship Staff","Ship Staff Insp.","Valve hydraulic deck penetration sleeves for COTS corroded/wasted.","Deck - Pipe / Fittings","General Appearance","Equipment Related","","","","","To creat a job in refman","2022-06-20","","Completed","2019-08-31","No","No","No","Internal"]
[null,null,null,null,3458,"23_2019-04-03 14:54:19.995","2019-07-08","Defect","Ship Staff","Ship Staff Insp.","IG VALVE OF SLP-S & 2C LEAKING","Inert Gas","General Appearance","Equipment Related","","","","","Slp-s changed and 2C found to be holding good","2019-09-07","","Completed","2019-09-04","No","No","No","Internal"]
[null,null,null,null,3459,"23_2019-04-04 14:54:19.995","2019-07-08","Defect","Ship Staff","Ship Staff Insp.","Both Anchor chain guide to hawse pipe and gypsy whelp wornout ","Miscellaneous","General Appearance","Equipment Related","","","","","to be built up  by welding and grinding. Job to entered in Refman","2019-11-20","","Completed","2019-09-04","No","No","No","Internal"]
[null,null,null,null,3373,"23_2019-07-30 14:54:19.995","2019-07-12","Defect","Ship Staff","Ship Staff Insp.","Crossover valve yellow line gear box hydraulic found leking","Deck - Pipe / Fittings","General Appearance","Equipment Related","","","","","COMPLETED","2019-07-17","","Completed","2019-07-15","No","No","No","Internal"]
[null,null,null,null,3374,"23_2019-07-31 14:54:19.995","2019-07-20","Defect","Ship Staff","Ship Staff Insp.","Mast riser cover found wasted and handle broken","Deck - Pipe / Fittings","General Appearance","Equipment Related","","","","","New cover fabricated and fixed in position by cold work","2019-07-31","","Completed","2019-07-30","No","No","No","Internal"]
[null,null,null,null,6713,"23_Sat Apr 06 2019 14:54:19 GMT+0000 (Coordinated Universal Time)","2019-07-25","Defect","Ship Staff","Ship Staff Insp.","5P WBT gauge reading is very erratic same to be purged frequently to get the correct reading","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.8","Medium","","","Overhauling carried out and tried, working satisfactory.","2019-09-30","","Completed","2019-09-05","No","No","No","Internal"]
[null,null,null,null,3445,"23_2019-05-21 14:54:19.995","2019-07-25","Defect","Ship Staff","Ship Staff Insp."," Main  IG line Dresser coupling near 5C pv valve  observe holed .","Deck - Pipe / Fittings","General Appearance","Equipment Related","","","","","Repaired and closed","2022-06-20","","Completed","2019-08-31","No","No","No","Internal"]
[null,null,null,null,3460,"23_2019-04-05 14:54:19.995","2019-07-25","Defect","Ship Staff","Ship Staff Insp.","Both side Pilot ladder reel  air motor pipe connection from operating box missing . ","Deck - Machinery","General Appearance","Equipment Related","","","","","A hose connection from gangway piping to be made for pilot ladder air motor","2019-09-08","","Completed","2019-09-02","No","No","No","Internal"]
[null,null,null,null,3461,"23_2019-04-06 14:54:19.995","2019-07-25","Defect","Ship Staff","Ship Staff Insp.","5P WBT gauge reading is very erratic same to be purged frequently to get the correct reading","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","Overhauling carried out and tried, working satisfactory.","2019-09-30","","Completed","2019-09-05","No","No","No","Internal"]
[null,null,null,null,3462,"23_2019-04-07 14:54:19.995","2019-07-25","Defect","Ship Staff","Ship Staff Insp.","Both gangway Air lubricator and Pumproom air lubricator found wasted, same to be renewed.","Deck - Machinery","General Appearance","Equipment Related","","","","","Gangway and fire wire reel changed","2019-09-08","DHAW190219","Completed","2019-09-06","No","No","No","Internal"]
[null,null,null,null,3438,"23_2019-05-14 14:54:19.995","2019-07-27","Defect","Ship Staff","Ship Staff Insp.","STBD lifeboat self lowering wire davit eye is broken, same replaced with a temporary cap arrangement.","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","HOOK WELDED","2019-08-20","","Completed","2019-08-24","No","No","No","Internal"]
[null,null,null,null,9950,"23_20/01/2020 6:37:47 PM","2019-07-27","Non Conformity","Ship Staff","Ship Staff Insp.","a crew made entry to pumproom without pumproom entry permit","Miscellaneous","ISM Related","Behaviour Based","5.2","Very High","","","Crew was immediately called out and permit was issued before he again went to pumproom.","2019-07-27","","Completed","2019-07-27","No","No","No","Internal"]
[null,null,null,null,3470,"23_2019-04-15 14:54:19.995","2019-07-28","Defect","Ship Staff","Ship Staff Insp.","8Nos COT  PV valve found leaking on pressure side ","Deck - Pipe / Fittings","General Appearance","Equipment Related","","","","","Overhauling of PV valves carried out no leaking PV valve found. ","2019-09-20","","Completed","2019-09-07","No","No","No","Internal"]
[null,null,null,null,3387,"23_2019-10-05 05:59:28.000","2019-07-29","Defect","Ship Staff","Ship Staff Insp.","EGB steam header outlet line pressure gauge to be calibrated","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","Will be carried out when Main Engine stopped/anchorage","2019-08-07","","Completed","2019-08-15","No","No","No","Internal"]
[null,null,null,null,3435,"23_2019-05-11 14:54:19.995","2019-07-29","Defect","Ship Staff","Ship Staff Insp.","Drinking water Hydrophore pump not developing pressure","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","PUMP NEED TO BE OVERHAULED","2019-08-15","","Completed","2019-08-19","No","No","No","Internal"]
[null,null,null,null,3443,"23_2019-05-19 14:54:19.995","2019-07-29","Defect","Ship Staff","Ship Staff Insp.","Accomadation Spare A/C compressor to be fixed on permanent base plate","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Hot work permit required,job will be carried out on Ballast passage.","2019-08-20","","Completed","2019-08-31","No","No","No","Internal"]
[null,null,null,null,3434,"23_2019-05-10 14:54:19.995","2019-08-01","Other","Ship Staff","Ship Staff Insp.","Packing materials to be added to Sox Scrubber tower","E/R - Main Engine","General Appearance","Equipment Related","","","","","Awaiting for spare supply.(SPARE PACKING MATERIALS RECEIVED ON 15-AUG-19)","2019-08-30","","Completed","2019-08-19","No","No","No","Internal"]
[null,null,null,null,9949,"23_20/01/2020 6:40:54 PM","2019-08-04","Defect","Ship Staff","Ship Staff Insp.","During port pre arrival checks the air hose for wilden pump found missing","Deck - Machinery","ISM Related","Knowledge Based","5.11","Low","","","A new air hose made and attached to wilden pump and marked only to be used for wilden pump.","2019-08-05","","Completed","2019-08-04","No","No","No","Internal"]
[null,null,null,null,3433,"23_2019-05-09 14:54:19.995","2019-08-08","Defect","Ship Staff","Ship Staff Insp.","No.2 Cargo Pump emergency stop not working from any of the emergency stop position.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","RECTIFIED","2019-09-08","","Completed","2019-08-19","No","No","No","Internal"]
[null,null,null,null,3446,"23_2019-05-22 14:54:19.995","2019-08-08","Defect","Ship Staff","Ship Staff Insp.","No.1 & No.2 WBP RPM control in CCR not working.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","COMPLETED","2019-09-08","","Completed","2019-08-20","No","No","No","Internal"]
[null,null,null,null,3447,"23_2019-05-23 14:54:19.995","2019-08-08","Defect","Ship Staff","Ship Staff Insp.","IG Pressure readout at Pumproom entrance is out by 400mmWG.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","Pressure gauge renewed.","2019-09-08","","Completed","2019-08-20","No","No","No","Internal"]
[null,null,null,null,3471,"23_2019-04-16 14:54:19.995","2019-08-08","Defect","Ship Staff","Ship Staff Insp.","IG pressure on deck readout in CCR is hunting in range of 100 mmWG and same is being printed as smudged line on printer.","Cargo Mach.","General Appearance","Equipment Related","","","","","Repairing on kinematic valve carried out and tested working satisfactory.","2019-09-08","","Completed","2019-09-26","No","No","No","Internal"]
[null,null,null,null,3690,"23_15/10/2019 6:37:24 AM","2019-08-09","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Bridge wing side support pillar derusting and painting\n\n","Accommodation","General Appearance","Human Error","11.8","Low","","","Both side bridge wing side support pillar derusting and painting completed  ","2019-10-25","","Completed","2019-10-25","No","No","No","Internal"]
[null,null,null,null,3436,"23_2019-05-12 14:54:19.995","2019-08-09","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","MSB unit cooler S.W.pipe line to replace with plastic pipes","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","COMPLETED","2019-08-23","","Completed","2019-08-19","No","No","No","Internal"]
[null,null,null,null,3439,"23_2019-05-15 14:54:19.995","2019-08-09","Defect","Ship Staff","Ship Staff Insp.","deck seal drain line one section to renew after deck seal","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","Renewed the leaky section. Satisfactory.","2019-08-25","","Completed","2019-08-27","No","No","No","Internal"]
[null,null,null,null,3440,"23_2019-05-16 14:54:19.995","2019-08-09","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Prov crane wire to renew, wire kinked near the top sheeve","Deck - Machinery","General Appearance","Equipment Related","","","","","Cable renewed with new spare. ","2019-08-25","","Completed","2019-08-27","No","No","No","Internal"]
[null,null,null,null,3448,"23_2019-05-24 14:54:19.995","2019-08-09","Defect","Ship Staff","Ship Staff Insp.","Steel plates and pipers around accom block, move to respective place in steering gear room","Accommodation","General Appearance","Equipment Related","","","","","Shifted to steering gear room","2019-08-25","","Completed","2019-08-22","No","No","No","Internal"]
[null,null,null,null,3449,"23_2019-05-25 14:54:19.995","2019-08-09","Defect","Ship Staff","Ship Staff Insp.","Few sections of Hydroblaster pipes to renew","Deck - Machinery","General Appearance","Equipment Related","","","","","Two lengths of damaged length renewed.","2019-08-25","","Completed","2019-08-19","No","No","No","Internal"]
[null,null,null,null,3450,"23_2019-05-26 14:54:19.995","2019-08-09","Defect","Ship Staff","Ship Staff Insp.","chair on bridge cover to repair","Accommodation","General Appearance","Equipment Related","","","","","Replaced with new chair.","2019-08-25","","Completed","2019-08-19","No","No","No","Internal"]
[null,null,null,null,3451,"23_2019-05-27 14:54:19.995","2019-08-09","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Two window frames cracked in Galley to replace with spares","Accommodation","General Appearance","Equipment Related","","","","","Replaced with spare","2019-08-25","","Completed","2019-09-01","No","No","No","Internal"]
[null,null,null,null,3455,"23_2019-05-31 14:54:19.995","2019-08-09","Defect","Ship Staff","Ship Staff Insp.","broken tiles on bridge toilet to repair","Accommodation","General Appearance","Equipment Related","","","","","Completed","2019-09-08","","Completed","2019-09-01","No","No","No","Internal"]
[null,null,null,null,3456,"23_2019-04-01 14:54:19.999","2019-08-09","Defect","Ship Staff","Ship Staff Insp.","old tube supports for bridge AC outside stbd door to remove and paint","Accommodation","General Appearance","Equipment Related","","","","","Completed","2019-09-08","","Completed","2019-09-01","No","No","No","Internal"]
[null,null,null,null,3463,"23_2019-04-08 14:54:19.995","2019-08-09","Defect","Ship Staff","Ship Staff Insp.","pallet trucks to overhaul and stow in IG room when not in use","Deck - Machinery","General Appearance","Equipment Related","","","","","Derusting in progress.","2019-09-08","","Completed","2019-09-07","No","No","No","Internal"]
[null,null,null,null,3466,"23_2019-04-11 14:54:19.995","2019-08-09","Defect","Ship Staff","Ship Staff Insp.","boiler water circ pump area, hydrophre pumps area and bulkheads ","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","Cleaning and painting.","2019-09-15","","Completed","2019-09-01","No","No","No","Internal"]
[null,null,null,null,3467,"23_2019-04-12 14:54:19.995","2019-08-09","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","FWG corner cosmetic upgradation reqd","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Bulkheads to clean and paint","2019-09-15","","Completed","2019-09-06","No","No","No","Internal"]
[null,null,null,null,3472,"23_2019-04-17 14:54:19.995","2019-08-09","Defect","Ship Staff","Ship Staff Insp.","both hose cranes cosmetic cleaning and painting","Deck - Machinery","General Appearance","Equipment Related","","","","","Completed","2019-09-30","","Completed","2019-09-28","No","No","No","Internal"]
[null,null,null,null,3474,"23_2019-04-18 14:54:19.995","2019-08-09","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Greasing on deck equipment","Deck - Mooring Machinery","General Appearance","Equipment Related","","","","","All deck equipment greasing completed","2019-09-30","","Completed","2019-09-30","No","No","No","Internal"]
[null,null,null,null,6652,"23_19/11/2019 10:30:26 PM","2019-08-12","Other","Ship Staff","Ship Staff Insp.","Steering gear room and forepeak store are full of old ropes and mooring tails.","Miscellaneous","General Appearance","Inappropriate Procedure","11.12","Low","","","Old mooring wires and ropes remvoed from steering gear and off-landed at Singapore on 05 Apr 2020 and area secured.","2020-02-15","","Completed","2020-04-06","No","No","No","Internal","arrange disposal in China this call or at Singapore along with supply barge."]
[null,null,null,null,3692,"23_15/10/2019 6:44:23 AM","2019-08-13","Defect","Ship Staff","Ship Staff Insp.","Meat room and Fish room doors found to have ice formation on door.","Accommodation","MLC Related","Equipment Related","11.13","Low","","","DHAW190211, Item no. 35 not received, new requisition raised DHAW190285\n\n\n\n","2019-11-07","DHAW190285","Completed","2019-11-04","No","No","No","Internal"]
[null,null,null,null,3452,"23_2019-05-28 14:54:19.995","2019-08-13","Defect","Ship Staff","Ship Staff Insp.","Hydroblaster pressure line from machine to forecastle, 3 length found damages.","Deck - Machinery","General Appearance","Equipment Related","","","","","To be changed after receiving stores","2019-08-20","","Completed","2019-08-22","No","No","No","Internal"]
[null,null,null,null,9218,"23_25/12/2019 4:17:08 AM","2019-08-15","Non Conformity","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Void Space of C-deck stbd aft of accommodation block found stored with chemical and paint pails. This is a non-designated space and all pails to be removed aft the space is ventilated and atmosphere checked. Enclosed space entry procedure to be followed.","Miscellaneous","ISM Related","Human Error","2.3","High","","","All the paints and chemicals removed from void space after following enclosed space procedure. All crew briefed about the dangers of enclosed space entry and the strict adherence to ESE permit checklist. Permission must be obtained from master for any Enclosed space entry.","2019-11-01","","Completed","2019-08-19","No","No","No","Internal"]
[null,null,null,null,9219,"23_25/12/2019 4:22:40 AM","2019-08-15","Non Conformity","Owner / Marine / Tech. Suptd.","Suptd. Insp.","For both lifeboats, floating hook top link and connecting chain of both Lifeboats to be de-rusted and crack test to be carried out at suspect locations (if any).","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.27","Medium","","","Derusting and painting carried out on connecting chain, no crack observed.","2019-11-01","","Completed","2019-08-23","No","No","No","Internal"]
[null,null,null,null,9220,"23_25/12/2019 4:28:24 AM","2019-08-15","Non Conformity","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Walkie Talkies not being used in accordance with Safety Flash 20180115 ‘Use and abuse of walkie-talkies on ships'.","Miscellaneous","ISM Related","Behaviour Based","4.26","Low","","","All crew informed to use the walkie talkie as per safety flash 20180115 during the safety meeting.","2019-11-01","","Completed","2019-08-29","No","No","No","Internal"]
[null,null,null,null,9221,"23_25/12/2019 4:35:29 AM","2019-08-15","Non Conformity","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Holed air hose being used on deck.","Deck - Machinery","General Appearance","Behaviour Based","","","","","Holed air hose removed from use and a new air hose placed on deck for use.","2019-11-01","","Completed","2019-08-19","No","No","No","Internal"]
[null,null,null,null,9222,"23_25/12/2019 4:42:53 AM","2019-08-15","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Rearrange Mid ship store so that the skylight opening can be used for lifting reducers.","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.12","Low","","","Space cleared by arranging the store for reducer lifting.","2019-11-01","","Completed","2019-08-23","No","No","No","Internal"]
[null,null,null,null,9223,"23_25/12/2019 8:19:54 AM","2019-08-15","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Greasing of P/S lifeboat davit wire and sheaves to be improved.","LSA / FFA","Safety / LSA / FFA","Human Error","5.28","Very High","","","Greasing of lifeboat fall wire and sheaves carried out after moving the lifeboat from stowed position.","2019-11-01","","Completed","2019-09-07","No","No","No","Internal"]
[null,null,null,null,9224,"23_25/12/2019 8:42:37 AM","2019-08-15","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","SOPEP gear to be removed from EHQ at stbd side.","Miscellaneous","General Appearance","Behaviour Based","11.13","Low","","","SOPEP gear removed from EHQ room stbd side and shifted to midship locker.","2019-11-01","","Completed","2019-08-16","No","No","No","Internal"]
[null,null,null,null,9225,"23_25/12/2019 8:47:29 AM","2019-08-15","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Pump room davit hook safety latch missing.","Deck - Machinery","Cargo / Ballast Systems","Equipment Related","5.2","Very High","","","A new safety latch fabricated and placed on hook.","2019-11-01","","Completed","2019-08-18","No","No","No","Internal"]
[null,null,null,null,9226,"23_25/12/2019 8:50:30 AM","2019-08-15","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","All deck officers to be familiarized with FPT bulkhead valve operation in Forecastle Store.","Miscellaneous","Crew Management","Knowledge Based","","","","","All deck crew familirised with the operation of FPT bulkhead valve operating procedure.","2019-11-01","","Completed","2019-09-05","No","No","No","Internal"]
[null,null,null,null,9227,"23_25/12/2019 8:53:29 AM","2019-08-15","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Hawse pipe cover sealing clamps found seized/broken.","Deck - Pipe / Fittings","ISPS Related","Equipment Related","7.12","High","","","Greasing of securing bolts are carried out and made free.","2019-11-01","","Completed","2019-08-16","No","No","No","Internal"]
[null,null,null,null,9228,"23_25/12/2019 8:56:45 AM","2019-08-15","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","All accommodation access doors to be checked for ability to lock and repair as required.","Accommodation","ISPS Related","Equipment Related","7.12","High","","","All doors checked for condition of locking and found to be in good condition.","2019-11-01","","Completed","2019-08-22","No","No","No","Internal"]
[null,null,null,null,9229,"23_25/12/2019 8:59:20 AM","2019-08-15","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Cut vegetables and other food products kept in Galley refrigerator without any cover.","Accommodation","MLC Related","Behaviour Based","11.13","Low","","","All the uncovered food products and cut vegetables covered ","2019-11-01","","Completed","2019-08-15","No","No","No","Internal"]
[null,null,null,null,9230,"23_25/12/2019 9:00:58 AM","2019-08-15","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Meat segregation keeping in view religious sentiments of seafarers on board not carried out in the reefer rooms.","Miscellaneous","MLC Related","Behaviour Based","11.13","Low","","","Meat were arranged in a manner that chicken are stowed on top which is consumed by all. Beef and Pork are stowed at bottom in different section so that these will not contaminate each other.","2019-11-01","","Completed","2019-08-20","No","No","No","Internal"]
[null,null,null,null,9237,"23_25/12/2019 1:27:35 PM","2019-08-15","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","M/E air cooler manometer water columns empty.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Main engine air cooler manometer water column filled with water. ","2019-11-01","","Completed","2019-08-21","No","No","No","Internal"]
[null,null,null,null,9238,"23_25/12/2019 1:30:48 PM","2019-08-15","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Gap at Pedestal grinder in E/R workshop found around 8 mm. Same to be maintained not above 2-3 mm.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","gap at pedestal grinder is adjusted and maintained about 3mm","2019-11-01","","Completed","2019-08-27","No","No","No","Internal"]
[null,null,null,null,6714,"23_Sun Apr 21 2019 14:54:19 GMT+0000 (Coordinated Universal Time)","2019-08-15","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Forward breast winch (S) #7 found leaking at control block.","Deck - Mooring Machinery","General Appearance","Equipment Related","9.14","Medium","","","O-rind changed for control lever. No more leak found.","2019-09-08","","Completed","2019-09-26","Yes","No","No","Internal"]
[null,null,null,null,6715,"23_Mon Apr 22 2019 14:54:19 GMT+0000 (Coordinated Universal Time)","2019-08-15","Defect","Ship Staff","Ship Staff Insp.","Meat room one hinge found broken.","Accommodation","General Appearance","Equipment Related","11.13","Low","","","One hinge fabricated and replaced","2019-09-30","","Completed","2019-09-20","No","No","No","Internal"]
[null,null,null,null,3442,"23_2019-05-18 14:54:19.995","2019-08-15","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","BILGES TANK TOP TO MAKE DRY OFF WATER AND PAINNT","Miscellaneous","General Appearance","Equipment Related","","","","","COMPLETED","2019-08-30","","Completed","2019-08-31","No","No","No","Internal"]
[null,null,null,null,3453,"23_2019-05-29 14:54:19.995","2019-08-15","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Spare floor plates on E-deck and pipes/ladder on D-deck to be placed in S/G Flat.","Accommodation","General Appearance","Equipment Related","","","","","Shifted to steering gear room.","2019-08-25","","Completed","2019-08-22","No","No","No","Internal"]
[null,null,null,null,3454,"23_2019-05-30 14:54:19.995","2019-08-15","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Airline valve on D-deck aft found leaking.","Deck - Pipe / Fittings","General Appearance","Equipment Related","","","","","Completed","2019-08-23","","Completed","2019-09-01","No","No","No","Internal"]
[null,null,null,null,3464,"23_2019-04-09 14:54:19.995","2019-08-15","Defect","Ship Staff","Ship Staff Insp.","Anchor wash port side 2 nozzle found chocked during anchor operation at singapore.","Deck - Machinery","General Appearance","Equipment Related","","","","","Pipes to be removed, cleaned and fixed back","2019-09-08","","Completed","2019-09-06","No","No","No","Internal"]
[null,null,null,null,3465,"23_2019-04-10 14:54:19.995","2019-08-15","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","BILGES TANK TOP TO MAKE DRY OFF WATER AND PAINT","Miscellaneous","General Appearance","Equipment Related","","","","","COMPLETED","2019-09-05","","Completed","2019-09-02","No","No","No","Internal"]
[null,null,null,null,3477,"23_2019-04-21 14:54:19.995","2019-08-15","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Forward breast winch (S) #7 found leaking at control block.","Deck - Mooring Machinery","General Appearance","Equipment Related","","","","","O-rind changed for control lever. No more leak found.","2019-09-08","","Completed","2019-09-26","Yes","No","No","Internal"]
[null,null,null,null,3478,"23_2019-04-22 14:54:19.995","2019-08-15","Defect","Ship Staff","Ship Staff Insp.","Meat room one hinge found broken.","Accommodation","General Appearance","Equipment Related","","","","","One hinge fabricated and replaced","2019-09-30","","Completed","2019-09-20","No","No","No","Internal"]
[null,null,null,null,3421,"23_2019-06-27 14:54:19.995","2019-08-16","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","HFO TRANSFER PUMP LEAKING AT SEAL","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","COMPLETED","2019-08-23","","Completed","2019-08-19","No","No","No","Internal"]
[null,null,null,null,3422,"23_2019-06-28 14:54:19.995","2019-08-16","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","DO TRANSFER PUMP LEAKING AT SEAL","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","COMPLETED","2019-08-23","","Completed","2019-08-19","No","No","No","Internal"]
[null,null,null,null,3423,"23_2019-06-29 14:54:19.995","2019-08-16","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","LO PURIFIER FEED PUMP LEAKING AT SEAL","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","COMPLETED","2019-08-23","","Completed","2019-08-19","No","No","No","Internal"]
[null,null,null,null,3424,"23_2019-06-30 14:54:19.995","2019-08-16","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","REMOTE START OF SOx SCRUBBER TO BE CONIRMED, ELSE SME T BE CAPTURED IN D&DRL","Elect. Mach. & Equip.","General Appearance","Equipment Related","","","","","CONFIRMED WORKING SATISFACTORILY ","2019-08-23","","Completed","2019-08-17","No","No","No","Internal"]
[null,null,null,null,3425,"23_2019-05-01 14:54:19.999","2019-08-16","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","E/R BOTTOM PLATFORM DOOR CLOSER OF EMERGENCY ESCAPE TO BE ADJUSTED","LSA / FFA","General Appearance","Equipment Related","","","","","COMPLETED","2019-08-17","","Completed","2019-08-17","No","No","No","Internal"]
[null,null,null,null,3426,"23_2019-05-02 14:54:19.995","2019-08-16","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","LEAK AT IG SCRUBBER FROM FLOAT FLANGE","Miscellaneous","General Appearance","Equipment Related","","","","","COMPLETED","2019-08-19","","Completed","2019-08-16","No","No","No","Internal"]
[null,null,null,null,3427,"23_2019-05-03 14:54:19.995","2019-08-16","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","LEAK AT DECK SEAL DRAIN LINE TO BE ARRESTED","Miscellaneous","General Appearance","Equipment Related","","","","","COMPLETED","2019-08-30","","Completed","2019-08-20","No","No","No","Internal"]
[null,null,null,null,3428,"23_2019-05-04 14:54:19.995","2019-08-16","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","AIRLINE VALVE ON D-DECK AFT FOUND LEAKING","Miscellaneous","General Appearance","Equipment Related","","","","","COMPLETED","2019-08-20","","Completed","2019-08-18","No","No","No","Internal"]
[null,null,null,null,3429,"23_2019-05-05 14:54:19.995","2019-08-16","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","SPARE FLOOR PLATES ON E-DECK AN DPIPES/LADDER ON D-DECK TO BE PLACED IN S/G FLAT","Miscellaneous","General Appearance","Equipment Related","","","","","COMPLETED","2019-08-30","","Completed","2019-08-19","No","No","No","Internal"]
[null,null,null,null,3430,"23_2019-05-06 14:54:19.995","2019-08-16","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","NO.2 COP EMERGENCY STOP NOT OPERATIONAL","Miscellaneous","General Appearance","Equipment Related","","","","","COMPLETED","2019-08-30","","Completed","2019-08-20","No","No","No","Internal"]
[null,null,null,null,3431,"23_2019-05-07 14:54:19.995","2019-08-16","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","E/R PORTABLE FOAM 20 LITRE CAN STICKER STATES \"VALID UNTIL 2018\"","Miscellaneous","General Appearance","Equipment Related","","","","","COMPLETED","2019-08-18","","Completed","2019-08-16","No","No","No","Internal"]
[null,null,null,null,3432,"23_2019-05-08 14:54:19.995","2019-08-16","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","E/R PORTABLE FOAM 20 LITRE CAN STICKER STATES \"VALID UNTIL 2018\"","Miscellaneous","General Appearance","Equipment Related","","","","","COMPLETED","2019-08-19","","Completed","2019-08-16","No","No","No","Internal"]
[null,null,null,null,3693,"23_14/10/2019 2:48:36 PM","2019-09-01","Defect","Ship Staff","Ship Staff Insp.","WBT remote reading deck purge unit top and bottom parts found badly corroded.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.8","Medium","","","Spare received and replacement done.","2020-01-27","DHAW190247","Completed","2020-04-15","No","No","No","Internal","spares confirmed for supply, check VFF and followup with procure"]
[null,null,null,null,6661,"23_19/11/2019 11:18:20 PM","2019-09-05","Defect","Ship Staff","Ship Staff Insp.","Lifeboat painter is very old and not in good condition, Lifeboat Tin opener, hatchet, turnbuckle not in good condition","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.29","High","","","Painter of both lifeboat renewed. Inventory of both lifeboat taken and all lifeboat equipments found in sufficient quantity and good condition.","2020-01-02","DHAW190268","Completed","2020-01-04","No","No","No","Internal"]
[null,null,null,null,3694,"23_14/10/2019 2:54:20 PM","2019-09-06","Defect","Ship Staff","Ship Staff Insp.","Control Valve for stbd gangway stowing winch found leaking.","Miscellaneous","ISPS Related","Equipment Related","5.47","Medium","","","Overhauled and inspected, found working satisfactory.","2020-01-25","DHAW190284","Completed","2020-04-10","No","No","No","Internal","arranged for supply in China this call."]
[null,null,null,null,3475,"23_2019-04-19 14:54:19.995","2019-09-06","Other","Ship Staff","Ship Staff Insp.","Arrangement for storing of lifting appliances to be made in midship store.","Miscellaneous","General Appearance","Equipment Related","","","","","Arrangement for lifting equipment storing made in midship store.","2019-09-30","","Completed","2019-09-24","No","No","No","Internal"]
[null,null,null,null,3476,"23_2019-04-20 14:54:19.995","2019-09-06","Defect","Ship Staff","Ship Staff Insp.","Back support for both midship crane operating platform found wasted.","Miscellaneous","General Appearance","Equipment Related","","","","","New support fabricated and fixed in position.","2019-09-25","","Completed","2019-09-30","No","No","No","Internal"]
[null,null,null,null,9190,"23_Wed Jun 12 2019 03:06:30 GMT+0000 (Coordinated Universal Time)","2019-09-10","Other","Ship Staff","Ship Staff Insp.","Helicopter equipment missing as per requirement. ","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.42","Medium","","","Inventory of helicopter equipment taken. List of equipments compared with helicopter guide. Missing items replaced from the store and inventory posted.","2020-01-20","RO- DHAW190268","Completed","2020-01-02","No","No","No","Internal"]
[null,null,null,null,3691,"23_15/10/2019 6:40:34 AM","2019-09-21","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","U clamps and bolts on deck lines to attend","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.5","Medium","","","Some of the U-clamps renewed and some which were in good condition, chipped/painted and box back with teflon.","2020-04-25","","Completed","2020-04-30","No","No","No","Internal","complete and close out prior arrival China mid Jan 20"]
[null,null,null,null,6663,"23_19/11/2019 11:28:00 PM","2019-09-25","Other","Ship Staff","Ship Staff Insp.","Scrubber tower doesn’t have portable fire fighting extinguisher.","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.42","Medium","","","Fire extinguishers for Scrubber tower received and same fixed in Scrubber tower.","2020-01-25","DHAW190288","Completed","2020-04-03","No","No","No","Internal","arranged for supply; followup with procure"]
[null,null,null,null,9951,"23_20/01/2020 6:43:01 PM","2019-09-28","Defect","Ship Staff","Ship Staff Insp.","Lock for harbour safety pin in open position for port side lifeboat was found wasted. ","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.28","Very High","","","Lock was fabricated and fixed in position.","2019-09-30","","Completed","2019-09-29","No","No","No","Internal"]
[null,null,null,null,6665,"23_19/11/2019 11:43:38 PM","2019-10-11","Defect","Ship Staff","Ship Staff Insp.","ODME fresh water supply doesn’t have stop valve. ","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","6.13","Low","","","Office informed by email, permission taken. pipeline removed.Valves fixed in position.","2019-11-30","","Completed","2019-11-26","No","No","No","Internal"]
[null,null,null,null,6666,"23_20/11/2019 12:03:37 AM","2019-10-15","Defect","Ship Staff","Ship Staff Insp.","Deck air line is in very bad condition","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","11.4","Very High","","","Derusting carried out from fwd upto midship store. Holed pipe section removed from location and built up work carried out. Same fixed back in locaiton after fabrication.","2020-03-01","","Completed","2020-04-07","No","No","No","Internal","one section renewed, no leaks now , other corroded sections to be renewed as well"]
[null,null,null,null,6653,"23_19/11/2019 10:20:33 PM","2019-10-15","Other","Ship Staff","Ship Staff Insp.","Vessel needs total 27 No.’s of USB locks (including 5 spare). Only10 USB locks are     onboard. Need 17 USB locks to meet the requirement as per message “All Ships - Please update on USB Locks - Annual review .","Accommodation ,Miscellaneous","Communication","Equipment Related","7.16","High","","","Office informed, awaiting supply","2020-01-25","","Completed","2020-01-25","No","No","No","Internal","supplied at Zhoushan on 24th and closed out"]
[null,null,null,null,6703,"23_21/11/2019 3:27:42 AM","2019-10-20","Defect","Ship Staff","Ship Staff Insp.","Bridge PC crashed and was temporarily replaced with stand alone PC in CCR which was for  Surveyor use.","Navigation - Others","Navigation","Equipment Related","4.7","High","","","New CPU received and same installed.","2020-02-25","","Completed","2020-03-10","No","No","No","Internal","RO 190326 was cancelled; raise fresh requisition from ship as per current requirement."]
[null,null,null,null,6669,"23_20/11/2019 12:16:32 AM","2019-10-24","Defect","Ship Staff","Ship Staff Insp.","Hydraulic motor for Winch MW3 is leaking","Deck - Machinery","Mooring","Equipment Related","9.15","Medium","","","reconditioned motor used to replace the leaking motor. New motor working satisfactory.","2020-01-02","","Completed","2019-12-04","No","No","No","Internal"]
[null,null,null,null,6670,"23_20/11/2019 12:21:50 AM","2019-10-24","Defect","Ship Staff","Ship Staff Insp.","Pumproom valve number BW-V813 is leaking.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.11","Medium","","","Oil seal of the valve actuator renewed and function test carried out. No leakage found.","2020-04-07","","Completed","2020-06-01","No","No","No","Internal","kindly update and revert with RO in the relevant box"]
[null,null,null,null,6671,"23_20/11/2019 12:24:07 AM","2019-10-24","Defect","Ship Staff","Ship Staff Insp.","Sludge transfer line from engine room to slop-S not in good condition.","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.4","Very High","","","Sludge line fabricated and fixed back in location.","2020-01-30","","Completed","2020-03-28","No","No","No","Internal","should have being closed out by now. date revised,"]
[null,null,null,null,6673,"23_20/11/2019 12:44:35 AM","2019-10-29","Defect","Ship Staff","Ship Staff Insp.","Stbd crane load testing to be carried out as wire was changed on 29 Oct 2019","Deck - Machinery","Cargo / Ballast Systems","External Factors","8.5","Very High","","","Load test of Stbd. mid ship crane carried out upto 11.5 tons.","2019-11-29","","Completed","2019-12-28","No","No","No","Internal","complete on priority. it should be done soon after any changes to crane or repairs; do not delay"]
[null,null,null,null,3689,"23_15/10/2019 6:30:57 AM","2019-10-29","Defect","Ship Staff","Ship Staff Insp.","No.2 Aux feed water pump not developing required pressure to maintain water level in Boiler","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Ohauled aux feed pump received from shore w/shop installed","2020-02-07","DHAW","Completed","2020-02-20","No","No","No","Internal","No issue with the pump while sailing and operating pressure below 10 bar. spares processed under 2020 office RO"]
[null,null,null,null,6674,"23_20/11/2019 12:46:51 AM","2019-11-01","Defect","Ship Staff","Ship Staff Insp.","Stbd side capstan air line is holed during last STS operation.","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.4","Very High","","","Wasted pipe of Stbd. capstan removed from location. New air inlet pipe for Stbd. capstan fabricated and fixed back in location.","2020-01-30","","Completed","2020-03-18","No","No","No","Internal","One leaking section repaired, one more corroded section to be replaced. Revised completion date to 30th Jan"]
[null,null,null,null,6675,"23_20/11/2019 12:50:05 AM","2019-11-03","Defect","Ship Staff","Ship Staff Insp.","Winch lever MW1 is slight hard to move.","Deck - Machinery","Mooring","Equipment Related","9.14","Medium","","","Overhauled and freed up.","2020-01-20","","Completed","2020-01-31","No","No","No","Internal","kindly attend and close out."]
[null,null,null,null,6676,"23_20/11/2019 12:54:52 AM","2019-11-06","Defect","Terminal Insp.","Terminal Insp.","5 nos Fire and 4 nos foam hydrants leaking.","LSA / FFA","Safety / LSA / FFA","Human Error","5.38","High","","","Replaced fire and foam hydrants.","2019-12-30","DHAW190325","Completed","2020-02-27","No","No","No","External","processed for supply, awaiting next convenient port"]
[null,null,null,null,6677,"23_20/11/2019 12:57:48 AM","2019-11-06","Defect","Ship Staff","Ship Staff Insp.","5P WBT gauge is found faulty","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.13","Medium","","","Requisition raised for new deck purge unit as same was found faulty.Replaced with new unit receievd at singapore, now working satisfactory.","2020-01-25","DHAW190314","Completed","2020-02-13","No","No","No","Internal","spares approved, awaiting supply"]
[null,null,null,null,6678,"23_20/11/2019 1:00:03 AM","2019-11-06","Defect","Ship Staff","Ship Staff Insp.","2 No.’s of COW machine is leaking from spindle.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.34","High","","","Greasing of all COW machines carried out. Defected COW machines of 3C COT tested and tried out during discharging operation at Kiire, Japan, all machines found to be working in good condition.","2020-02-10","","Completed","2020-03-29","No","No","No","Internal","OH in ballast leg and close out"]
[null,null,null,null,6681,"23_20/11/2019 1:12:14 AM","2019-11-08","Defect","Ship Staff","Ship Staff Insp.","Lifeboat safety belts buckle jammed, port Lifeboat port side coxswain safety belt broken","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.27","Medium","","","Lifeboat safety belt buckle freed up and coxwain safety belt on port lifeboat renewed.","2019-11-20","","Completed","2019-11-19","No","No","No","Internal","it takes less time to complete the job rather then leaving open in the DDRL. close out on priority"]
[null,null,null,null,6682,"23_20/11/2019 2:00:31 AM","2019-11-08","Defect","Ship Staff","Ship Staff Insp.","Stbd lifeboat Brake need external force to apply brake once it is heaved up for lowering.","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.28","Very High","","","Brake assembly opened found rust deposit . Same cleaned and brake assembly boxed back. Lifeboat lowered and brake tested for operation. All found satisfactory.","2019-11-25","","Completed","2019-11-24","No","No","No","Internal","reported to be completed , show completed...."]
[null,null,null,null,6683,"23_20/11/2019 3:21:39 AM","2019-11-11","Other","Ship Staff","Ship Staff Insp.","Intrinsically safe camera’s charging port is slightly damaged . Screen minor damage. Cable pin is broken.SIM card & charger is Missing.","Critical Equip.,Miscellaneous","Communication","Behaviour Based","5.6","Low","","","Lumix Camera supplied at Singapore.","2020-01-30","","Completed","2020-02-07","No","No","No","Internal","raise RO for spare cable and charger"]
[null,null,null,null,6696,"23_21/11/2019 2:57:25 AM","2019-11-11","Defect","Ship Staff","Ship Staff Insp.","No.1 Steering gear hydraulic pump minor weeping  from seal.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Seals repalced with new one by shore contractor.","2020-01-30","DHAW190322","Completed","2020-02-18","No","No","No","Internal","spares confirmed for supply. to complete the job once the spares are received and report back. awaiting connection"]
[null,null,null,null,6698,"23_21/11/2019 3:01:00 AM","2019-11-11","Defect","Ship Staff","Ship Staff Insp.","Control block's end cover of port aft spring winch is holed.","Deck - Mooring Machinery","Mooring","Equipment Related","9.15","Medium","","","Control block end cover remvoed. Fabrication carried out and fixed back in postion. Leak arrested and found satisfactory.","2020-02-25","DHAW190316","Completed","2020-04-01","No","No","No","Internal","spares processed; have long lead time, expected end Feb"]
[null,null,null,null,6700,"23_21/11/2019 3:13:04 AM","2019-11-11","Defect","Ship Staff","Ship Staff Insp.","Drinking water pump need to be overhauled. Mineralizer chemical need to ordered. ","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","11.1","High","","","rectified","2019-12-30","","Completed","2019-11-23","No","No","No","Internal","plan for new sterilizer unit soon. in the mean time chem will be supplied"]
[null,null,null,null,6684,"23_20/11/2019 4:32:27 AM","2019-11-12","Defect","Ship Staff","Ship Staff Insp.","Isolation valve for MW2 is not able to close due to wasted closing screw","Deck - Mooring Machinery","Mooring","Equipment Related","9.14","Medium","","","Spare received, isolation valve replaced, tested and found satisfactory.","2020-01-30","DHAW190321","Completed","2020-04-08","No","No","No","Internal","follow up with separate mail and condition report. spares confirmed for supply.\n18th Jan: Spare will be ready on 31st Jan."]
[null,null,null,null,6685,"23_20/11/2019 4:35:35 AM","2019-11-12","Defect","Ship Staff","Ship Staff Insp.","2 wasted platform near IG isolation valve.","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.4","Very High","","","New grating fabricate and fix back","2020-02-15","","Completed","2020-02-25","No","No","No","Internal","please completed before revised target time"]
[null,null,null,null,6686,"23_20/11/2019 4:39:35 AM","2019-11-12","Defect","Ship Staff","Ship Staff Insp.","Hydroblaster line on deck rubber coating failure at two places.","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.4","Very High","","","Damaged hydroblaster hoses replaced with the new one present onboard. Requisition has been raised to replenish the onboard quantity.","2020-01-02","DHAW190319","Completed","2019-12-27","No","No","No","Internal","processed supply,"]
[null,null,null,null,6687,"23_20/11/2019 4:42:01 AM","2019-11-12","Defect","Ship Staff","Ship Staff Insp.","Deck valve handwheel wasted at numerous locations","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.4","Very High","","","Broken handwheels replaced with spares onboard. ","2020-01-30","DHAW190255","Completed","2020-04-14","No","No","No","Internal","this should be closed the very next day it is noticed. why is it left open. quantify how many handles are broken. \n18 Jan: Please raise a fresh RO as PO 190255 of Deck store was closed."]
[null,null,null,null,6688,"23_20/11/2019 4:43:44 AM","2019-11-12","Defect","Ship Staff","Ship Staff Insp.","Deck boxes for Lifebuoy light wasted","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.4","Very High","","","Wasted box removed from location and fabrication carried out.","2020-01-30","","Completed","2020-02-25","No","No","No","Internal","to be completed before target time"]
[null,null,null,null,6689,"23_20/11/2019 5:08:04 AM","2019-11-12","Defect","Ship Staff","Ship Staff Insp.","C- Deck and D-deck alleyway door lock to be rectified. Both Sides (Port & Stbd).","Accommodation","General Appearance","Equipment Related","11.6","Medium","","","New doors were fixed on C & D Deck alleyway. Presently these doors are shutting but door lock hole in bulkhead in not matching with the old one. New Holes fabricated and fixed on C & D-deck.","2019-12-20","","Completed","2019-11-26","No","No","No","Internal"]
[null,null,null,null,6690,"23_20/11/2019 5:09:41 AM","2019-11-12","Defect","Ship Staff","Ship Staff Insp.","Chief Cook cabin porthole frame is cracked","Accommodation","General Appearance","Equipment Related","11.6","Medium","","","Replace the same with spare onboard","2019-12-20","","Completed","2019-11-20","No","No","No","Internal","reported to be close,"]
[null,null,null,null,6691,"23_20/11/2019 5:12:41 AM","2019-11-12","Defect","Ship Staff","Ship Staff Insp.","Valve hydraulic box No.3 leak at pipe","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.11","Medium","","","Leak is from small crack on welding. Presently repaired by soft patch. Permanent repair not possible as these pipes are welded to the box. After soft patch no leak observed. ","2019-11-30","","Completed","2019-11-26","No","No","No","Internal","awaiting more details from ship for onboard repairs"]
[null,null,null,null,6706,"23_21/11/2019 3:34:46 AM","2019-11-13","Defect","Ship Staff","Ship Staff Insp.","X-Band Radar TXRX Fan nearing Life expectancy.","Navigation - RADAR","Navigation","Equipment Related","4.7","High","","","TXRX fan replaced.","2020-01-30","DHAW190329","Completed","2020-02-06","No","No","No","Internal","spares onboard;.  kindly check and revert why it is open"]
[null,null,null,null,9216,"23_25/12/2019 3:53:25 AM","2019-11-14","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Some Garbage bins kept in Accommodation and at Garbage station not color coded as per the Garbage Management plan.","Miscellaneous","ISM Related","Human Error","6.2","High","","","All garbage bins in accommodation and at garbage receptacle area correctly color coded and marked as per Garbage Management Plan.","2020-02-14","","Completed","2019-12-19","No","No","No","Internal"]
[null,null,null,null,9217,"23_25/12/2019 3:58:22 AM","2019-11-14","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Some of the Jobs for LSA / FFA maintenance is updated in PAL PMS only as Satisfactory without any description of work carried out. Also No LSA / FFA Maintenance Record is being maintained onboard","Miscellaneous","ISM Related","Human Error","10.12","Very High","","","All officers and engineers briefed on the procedure of completing the PMS in PAL system. All officers and engineers informed to attach photos, checklist and RA to pms jobs as applicable.","2020-02-14","","Completed","2019-12-17","No","No","No","Internal"]
[null,null,null,null,9234,"23_25/12/2019 1:11:02 PM","2019-11-14","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Main Engine Unit no 5 and 6 having leaks near the High pressure pipes of Fuel valve and have containers placed to collect the leak.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.19","Very High","","","main engine unit no.5 and 6 fuel valve high pressure pipe leak rectified.","2020-02-14","","Completed","2019-12-01","No","No","No","Internal"]
[null,null,null,null,9236,"23_25/12/2019 1:21:20 PM","2019-11-14","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Old oil stains observed near the purifier area and requires cleaning and painting.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.2","Low","","","oil stains cleaned and purifier area painted.","2020-12-14","","Completed","2019-11-22","No","No","No","Internal"]
[null,null,null,null,9239,"23_24/12/2019 10:33:48 PM","2019-11-14","Non Conformity","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Safety contour and Safety Depth values wrongly calculated in passage plan from Erha to San Diego, San Diego to PAL, PAL to Long Beach Anchorage and Long Beach Anchorage to Berth.","Navigation - Others","Navigation","Human Error","4.15","Very High","","","Correct values calculated & entered in the form.Safety contour and Safety Depth values to always double check to avoid incorrect information. It must be cross checked by all other officers including master.","2020-02-14","","Completed","2019-11-15","No","No","No","Internal"]
[null,null,null,null,9240,"23_25/12/2019 1:52:20 PM","2019-11-14","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Company Standing Orders were not countersigned by Watch keeping Ratings.","Navigation - Others","Navigation","Human Error","4.2","Medium","","","Company Standing Orders were read & countersigned by all Watch keeping Ratings. Meeting conducted with all deck officers and ratings and everyone informed to ensure positive compliance. This information to be passed on to their relievers to prevent recurrence.","2020-02-14","","Completed","2019-11-15","No","No","No","Internal"]
[null,null,null,null,9241,"23_25/12/2019 2:05:52 PM","2019-11-14","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Similar Engine Speed for Ahead and Astern is mentioned in the Pilot card","Navigation - Others","Navigation","Human Error","4.7","High","","","Correct ahead and astern speeds to be mentioned in pilot card.","2020-02-14","","Completed","2019-11-30","No","No","No","Internal"]
[null,null,null,null,9952,"23_20/01/2020 5:21:01 PM","2019-11-14","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Chief Officer did not keep even One Bridge watch in a Day from 15th Oct to 29th Oct when the vessel was in Open Seas.","Miscellaneous","Crew Management","Behaviour Based","","","","","Work planning was changed and chief officer started going for bridge watch.","2020-02-14","","Completed","2019-11-26","No","No","No","Internal"]
[null,null,null,null,9953,"23_20/01/2020 5:24:07 PM","2019-11-14","Non Conformity","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Lifeboat and Fire Drill is required to be carried out weekly as per the Drill Schedule. However this was not complied with in the month of Aug, Sept and Oct 2019. Also Rescue from Enclosed Space drill was not carried out for Oct 2019.","Miscellaneous","ISM Related","Inappropriate Procedure","5.14","Very High","","","Drills are being carried out as per Drill schedule. Vessel is strictly ensuring compliance as required.","2020-02-14","","Completed","2019-11-16","No","No","No","Internal"]
[null,null,null,null,9194,"23_25/12/2019 3:01:06 AM","2019-11-14","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Fwd and Aft mooring area Anti Skid paint completely worn out and needs to be Re-painted with Anti Skid","Deck - Mooring Machinery","Mooring","Human Error","9.14","Medium","","","Fwd and aft mooring area re-painted with anti skid.","2020-02-14","","Completed","2020-05-11","No","No","No","Internal","vessel to raise RO for paint supply at Singapore ,ETA end Jan"]
[null,null,null,null,9195,"23_25/12/2019 3:04:44 AM","2019-11-14","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Snap back Zones stencil at various locations faded or overpainted","Deck - Mooring Machinery","Mooring","Human Error","9.19","Low","","","Snap Back zones re-painted and clearly stencilled.","2020-02-14","","Completed","2020-01-03","No","No","No","Internal"]
[null,null,null,null,9196,"23_25/12/2019 3:31:27 AM","2019-11-14","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Cargo and Bunker Sample Log Not maintained onboard","Miscellaneous","Cargo / Ballast Systems","Human Error","8.17","Low","","","Cargo and bunker sample log maintained and kept updated onboard.","2020-02-14","","Completed","2019-12-29","No","No","No","Internal"]
[null,null,null,null,9197,"23_25/12/2019 4:02:31 AM","2019-11-14","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Record of Lifting Gear not updated for 2019","Miscellaneous","ISM Related","Human Error","10.28","Low","","","Record of Lifting Gear updated and all lifting appliances marked and tagged as per the inventory.","2020-02-14","","Completed","2020-01-04","No","No","No","Internal","to complete on priority. \nship has load cell onboard. kindly complete and close out on priority"]
[null,null,null,null,9198,"23_25/12/2019 4:09:24 AM","2019-11-14","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Numerous Manholes on deck require Stenciling to Indicate the spaces served.","Hull & Tanks","General Appearance","Behaviour Based,Human Error","11.3","Medium","","","All manholes on deck stenciled to indicate the spaces served.","2020-02-14","","Completed","2020-01-07","No","No","No","Internal"]
[null,null,null,null,9201,"23_25/12/2019 12:59:33 PM","2019-11-14","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Hydraulic oil, minor oil leaking from No 2 Steering Gear pump","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.39","High","","","Steering gear pump seal replaced by shore contractor","2020-02-14","DHAW190322","Completed","2020-02-18","No","No","No","Internal","Spares under PO 190322 is ready now and will be connected to next convenient port. Meantime, please closely monitor the leak and inform office is it is excessive and may affect the steering."]
[null,null,null,null,9207,"23_24/12/2019 10:40:06 PM","2019-11-14","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Provision Store (Wet and Dry) requires cleaning, tidying up and arrangement of Provisions","Accommodation","General Appearance","Behaviour Based","11.13","Low","","","Provision Store (Wet and Dry) to be cleaned and  arranged.","2020-02-14","","Completed","2019-12-07","No","No","No","Internal"]
[null,null,null,null,9208,"23_24/12/2019 10:46:48 PM","2019-11-14","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Restricted areas not marked as per 06.02 of SSP","Accommodation","ISPS Related","Human Error","7.12","High","","","All areas to be checked as per SSP and Missing stencil on door to be marked. ","2020-02-14","","Completed","2019-12-09","No","No","No","Internal"]
[null,null,null,null,9209,"23_24/12/2019 10:51:24 PM","2019-11-14","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Crew and Officers Laundry requires cleaning, tidying up.","Accommodation","General Appearance","Behaviour Based","11.13","Low","","","Crew & officer laundry cleaning & painting to be carried out. Unnecessary items removed from laundry.","2020-02-14","","Completed","2019-11-22","No","No","No","Internal"]
[null,null,null,null,9210,"23_24/12/2019 10:58:43 PM","2019-11-14","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Brake rendering marking on the Mooring winch is not clear regarding the set point value.","Deck - Mooring Machinery","Mooring","Human Error","9.7","Medium","","","Break rendering mark on the mooring winch to be marked and highlighted correctly.","2020-02-14","","Completed","2019-12-18","No","No","No","Internal"]
[null,null,null,null,9211,"23_25/12/2019 3:08:17 AM","2019-11-14","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Heavy rust on the mooring bollards and the SWL Bead weld marking not highlighted.","Deck - Mooring Machinery","Mooring","Human Error","9.19","Low","","","All bollards de-rusted and painted. All SWL bead weld marking highlighted.","2020-02-14","","Completed","2019-12-19","No","No","No","Internal"]
[null,null,null,null,9212,"23_25/12/2019 3:23:44 AM","2019-11-14","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","CCR Logbook not completely filled up for all the entries as required by the instructions given at the beginning of the book for PAL and Long Beach with Master’s signature missing.","Documentation","Cert. & Docu.","Human Error","4.2","Medium","","","All officers are briefed for compliance and entries are being made as per the instructions given at the beginning of CCR log. Master signature is entered atleast once in 12 hrs.","2020-02-14","","Completed","2019-12-14","No","No","No","Internal"]
[null,null,null,null,9213,"23_25/12/2019 3:36:41 AM","2019-11-14","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Emergency Port contact list for current port not posted in CCR and Bridge","Miscellaneous","Communication","Human Error","6.1","Medium","","","Emergency Port contact list for current port posted in CCR and Bridge.","2020-02-14","","Completed","2019-12-13","No","No","No","Internal"]
[null,null,null,null,9214,"23_25/12/2019 3:39:25 AM","2019-11-14","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Lagging missing or in poor condition near the Stripper pump in Pumproom","Cargo Mach.","Cargo / Ballast Systems","Behaviour Based","8.8","Medium","","","Old lagging on steam line of stripping pump removed and replaced by new lagging.","2020-02-14","","Completed","2019-12-19","No","No","No","Internal"]
[null,null,null,null,9215,"23_25/12/2019 3:51:05 AM","2019-11-14","Non Conformity","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Garbage record book not signed by the Officer in-charge (2nd Engineer) for entries relating to Incineration of Garbage since May 2019. Same only signed by Chief Officer.","Miscellaneous","ISM Related","Human Error","6.2","High","","","All garbage incineration enteries counter signed by 2nd Engineer.","2020-02-14","","Completed","2019-12-03","No","No","No","Internal"]
[null,null,null,null,6692,"23_20/11/2019 5:14:26 AM","2019-11-16","Defect","Ship Staff","Ship Staff Insp.","Filter for Valve hydraulic box on deck is wasted at bottom","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.11","Medium","","","Filter inspected and cleaned. Filter fixed back in location and found satisfactory.","2020-01-30","DHAW190318","Completed","2020-04-09","No","No","No","Internal","spares processed, complete upon receipt of spares"]
[null,null,null,null,6693,"23_20/11/2019 5:17:01 AM","2019-11-16","Defect","Ship Staff","Ship Staff Insp.","Winch MW 02 control lever leaking near seal","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.11","Medium","","","Control lever overhauled and inspected. Oil seal renewed and control lever fixed back in location, found satisfactory.","2020-01-31","","Completed","2020-04-10","No","No","No","Internal","awaiting further feedback from ship, if required place RO for the spares"]
[null,null,null,null,6707,"23_21/11/2019 3:38:09 AM","2019-11-16","Defect","Ship Staff","Ship Staff Insp.","Port lifeboat air cylinder charging hose is leaking at connection","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.24","Very High","","","Damaged hose replaced with the new one received.","2020-02-10","DHAW190330","Completed","2020-04-16","No","No","No","Internal","connected onboard ship- kindly complete the job  and close out"]
[null,null,null,null,6708,"23_21/11/2019 4:46:40 AM","2019-11-16","Defect","Ship Staff","Ship Staff Insp.","IG LINE CRACKED AT SUPPORT NEAR 5C COT","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","11.4","Very High","","","Temporary Repair carried out . No leak observed. Permanent repairs will be carried out in DD. Observation entered in REFMAN.","2022-09-26","","Completed","2020-09-01","Yes","No","No","Internal","Make repair specs in refman and carry out temp repairs again as suggested / forward the repair spec in REFMAN and close out"]
[null,null,null,null,9954,"23_20/01/2020 6:19:12 PM","2019-11-17","Non Conformity","Ship Staff","Ship Staff Insp.","During Accomodation inspection, Found some of the common places garbage bin not colour coded as required by Garbage Management Plan.","Accommodation","MARPOL Related","Inappropriate Procedure","6.2","High","","","Garbage Bins colour coded to comply with Garabge Management Plan.","2019-12-31","","Completed","2019-12-10","No","No","No","Internal"]
[null,null,null,null,6651,"23_19/11/2019 10:25:32 PM","2019-11-17","Defect","Ship Staff","Ship Staff Insp.","Cargo sampler onboard is not closed type.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.16","Very High","","","New Cargo sampler received at Singapore.","2020-01-30","DHAW20009","Completed","2020-05-24","No","No","No","Internal","Raise RO for supply at Singapore next call in end of January. /"]
[null,null,null,null,9231,"23_25/12/2019 10:06:37 AM","2019-11-20","Non Conformity","Ship Staff","Nav Audit / Verification","Found few overwriting for wrong entries in Deck Log Book. ","Navigation - Others","Navigation","Human Error","4.2","Medium","","","Correct entry made on top & intialled.","2019-12-31","","Completed","2019-11-20","No","No","No","Internal"]
[null,null,null,null,9232,"23_25/12/2019 10:11:24 AM","2019-11-20","Non Conformity","Ship Staff","Nav Audit / Verification","Found laminated watch handover checklist 12.01.35.041.01 dated previous date and not dated to correct date for one Navigation Watch.\n\n","Navigation - Others","Navigation","Human Error","4.2","Medium","","","Correct date entered .","2019-12-31","","Completed","2019-11-20","No","No","No","Internal"]
[null,null,null,null,9233,"23_25/12/2019 10:14:40 AM","2019-11-20","Non Conformity","Ship Staff","Nav Audit / Verification","Found few Navtex messages not signed by all officers.","Navigation - GMDSS & Communication","Navigation","Human Error","4.13","Very High","","","Concerned officers acknowledged and signed.","2019-12-31","","Completed","2019-11-20","No","No","No","Internal"]
[null,null,null,null,3685,"23_15/10/2019 5:59:28 AM","2019-12-01","Defect","Ship Staff","Ship Staff Insp.","Old control air dryer to be installed parallel with new control air dryer","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","11.1","High","","","Installed air dryer","2020-07-22","","Completed","2020-08-25","No","No","No","Internal","kindly complete after departure Zirku"]
[null,null,null,null,9955,"23_20/01/2020 5:42:47 PM","2019-12-01","Non Conformity","Ship Staff","Ship Staff Insp.","Entry of BANWAS status was not found in Bridge Bell Book after Vessel moored @ berth 121 Long Beach.","Documentation","Navigation","Human Error","4.2","Medium","","","Missing Entry made in Bridge Bell Book.","2019-12-31","","Completed","2019-12-01","No","No","No","Internal"]
[null,null,null,null,9202,"23_Wed Jun 12 2019 18:57:34 GMT+0000 (Coordinated Universal Time)","2019-12-01","Defect","Ship Staff","Ship Staff Insp.","During STS operation at PAL suspected No.2 manifold valve stbd side leaking.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","11.4","Very High","","","Old seat ring renewed with spare seat ring onboard. Pressure test carried with compressed air to 7 bar holding correctly.","2019-12-10","","Completed","2019-12-10","No","No","No","Internal"]
[null,null,null,null,9192,"23_13/12/2019 11:25:24 PM","2019-12-13","Defect","Ship Staff","Ship Staff Insp.","Minerals need to be added in drinking water line. One dosing pump is working and another one is on order.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Dosing pump installed ,mineraliser working satisfactory , both chlorine and mineral dosing pump working in auto mode","2020-05-25","DHAW190327","Completed","2020-05-31","No","No","No","Internal","spares supplied, kindly take action and close out"]
[null,null,null,null,9193,"23_21/12/2019 6:39:36 AM","2019-12-15","Breakdown","Ship Staff","Ship Staff Insp.","During mooring operation observed oil leaks through the shaft seal.","Deck - Mooring Machinery","Mooring","Equipment Related","9.14","Medium","","","Motor overhauled and shaft seal renewed, tested no leaks observed all working satisfactoy.","2020-06-15","","Completed","2020-01-31","No","No","No","Internal","Understand seal renewal is in progress and expect to complete before arrival China on 22nd Jan. Please update office about the completion. Please add the PO number."]
[null,null,null,null,9203,"23_21/12/2019 6:47:56 AM","2019-12-16","Defect","Ship Staff","Ship Staff Insp.","During testing of main engine, observed No.5 and No.7 unit, starting air valve air inlet flange gasket leaks.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Both gaskets renewed after stopping the engine. and engine tried out, no leaks observed.","2019-12-20","","Completed","2019-12-18","No","No","No","Internal"]
[null,null,null,null,9235,"23_25/12/2019 1:17:25 PM","2019-12-18","Defect","Ship Staff","Ship Staff Insp.","Main engine starting air line drain valve leaking .","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Main engine starting air line drain valve found leaking, same removed observed union crack, same  renewed with spare .","2019-12-25","","Completed","2019-12-23","No","No","No","Internal"]
[null,null,null,null,9204,"23_21/12/2019 7:01:47 AM","2019-12-18","Defect","Ship Staff","Ship Staff Insp.","During routine inspection of main engine exhaust manifold it is observed that lagging for manhole cover was not in place.","E/R - Main Engine","Eng. / Strg. Comp.","Knowledge Based","10.32","Very High","","","After completing inspection fabricated and fixed new lagging. ","2019-12-20","","Completed","2019-12-18","No","No","No","Internal"]
[null,null,null,null,9205,"23_21/12/2019 7:16:53 AM","2019-12-20","Defect","Ship Staff","Ship Staff Insp.","Railing near main engine cylinder head platform found moving free as its securing arrangement found parted.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","External Factors","10.1","Medium","","","Hand railing securing arrangement fixed. ","2019-12-21","","Completed","2019-12-20","No","No","No","Internal"]
[null,null,null,null,9206,"23_21/12/2019 7:22:17 AM","2019-12-20","Defect","Ship Staff","Ship Staff Insp.","During routine check of scavenge drain tank. It is observed that drain valve was chocked.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.11","Medium","","","Cleared the valve after removing the flange connection.","2019-12-21","","Completed","2019-12-20","No","No","No","Internal"]
[null,null,null,null,9189,"23_Wed Jun 12 2019 19:55:23 GMT+0000 (Coordinated Universal Time)","2020-01-01","Defect","Ship Staff","Ship Staff Insp.","Deck crossover valve CO V507 found leaking","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","11.4","Very High","","","Valve open/ shut several times and found all in order. No leak observed.","2020-04-15","","Completed","2020-04-30","No","No","No","Internal","Kindly mention the RO in the defect list and followup with procure.\n18th Jan: Have you raised RO? Add the RO number in DDRL. Plan OH during the ballast leg to Singapore"]
[null,null,null,null,9443,"23_06/01/2020 7:55:18 AM","2020-01-02","Observation","Ship Staff","Ship Staff Insp.","COPT condenser cooling sea water pump 1 sacrificial anode cover found leaking.","Cargo Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Pump isolated, drained and anode cover removed. Cover repaired by welding in workshop and put back in place.","2020-01-03","","Completed","2020-01-02","No","No","No","Internal"]
[null,null,null,null,9444,"23_06/01/2020 10:19:08 AM","2020-01-02","Observation","Ship Staff","Ship Staff Insp.","Galley package AC condenser cooling sea water inlet line found leaking.","Accommodation ","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Galley AC stopped and cooling sea water to condensor isolated. Pipe and condensor removed from place . Welding carried out on both sea water inlet and outlet pipes.","2020-01-06","","Completed","2020-01-03","No","No","No","Internal"]
[null,null,null,null,3688,"23_15/10/2019 6:28:34 AM","2020-01-08","Defect","Ship Staff","Ship Staff Insp.","IG Valve  2C leaking.","Inert Gas","Cargo / Ballast Systems","Equipment Related","8.31","High","","","Spare received valve was not correct size so raised new RO & Raised defect with new date","2020-08-08","DHAW205012","Completed","2020-10-02","No","No","No","Internal","spares arranged for supply, close out on receipt.\nof spares. complete after departure Korea and prior arrival Singapore"]
[null,null,null,null,9511,"23_10/01/2020 8:41:57 AM","2020-01-09","Defect","Ship Staff","Ship Staff Insp.","V.D.R is recording from all 75 channels but no video  recording available for X-band Radar,S-band Radar,ECDIS No.1 & ECDIS No.2","Navigation - VDR / BNWAS","Navigation","Equipment Related","","","","","Office informed . Defects identified. Awaiting supply of required parts to rectify defects.","2020-02-09","","Completed","2020-01-25","No","No","No","Internal","Trouble shooting done. Job is considered closed .DC converter is supplied and fitted in place. 24 Jan Zhoushan"]
[null,null,null,null,9937,"23_20/01/2020 7:32:21 PM","2020-01-14","Defect","Ship Staff","Ship Staff Insp.","BNWAS back-up battery is not getting charged as battery is defective.","Navigation - VDR / BNWAS","Navigation","Equipment Related","","","","","Battery received in Singapore and replaced to BNWAS.","2020-02-10","DHAW 200004","Completed","2020-02-09","No","No","No","Internal","the system is in operational condition. spare battery will be processed for supply at Singapore this call"]
[null,null,null,null,9938,"23_20/01/2020 7:23:32 PM","2020-01-14","Defect","Ship Staff","Ship Staff Insp.","Fluorecent light globe/shade has lot of hairline crack.","Elect. Mach. & Equip.","Emgcy. Systems","Equipment Related","10.37","Medium","","","Light shades replaced where required.","2020-04-20","DHAW 190317","Completed","2020-04-22","No","No","No","Internal","could not be arranged in China due to logistic shut down ( chinese new yera)\nrearranged at singapore around 08th Feb/ spares on board - work was in progress, complete and close out"]
[null,null,null,null,10627,"23_14/02/2020 4:24:15 PM","2020-01-25","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Fish room door handle broken","Accommodation","MLC Related","Equipment Related","11.13","Low","","","Fish room broken handle replaced.","2020-03-24","","Completed","2020-04-11","No","No","No","Internal"]
[null,null,null,null,10628,"23_14/02/2020 4:40:23 PM","2020-01-25","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Stbd windlass Big gear top cover, one aft section part wasted, to renew","Deck - Mooring Machinery","Mooring","Equipment Related","9.2","Very High","","","Stbd windlass gypsy wasted cover removed /fabricated and box back.","2020-05-25","","Completed","2020-09-15","No","No","No","Internal","noted the damaged section renewed, close out and raise defect in refman"]
[null,null,null,null,10629,"23_14/02/2020 5:05:50 PM","2020-01-25","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Change lockers and main deck alley way paint light green and complete white paint on the bulkheads to improve appearance ","Accommodation","General Appearance","Equipment Related","11.13","Low","","","Painting of Upper deck alleyway and bulkheads carried out.","2020-02-10","","Completed","2020-02-20","No","No","No","Internal"]
[null,null,null,null,10630,"23_14/02/2020 4:28:25 PM","2020-01-25","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Pump room machinery and frames have settled dust, needs good cleaning","Cargo Mach.","Cargo / Ballast Systems","Behaviour Based","8.51","Low","","","Pumproom machinery and frames cleaned properly","2020-02-10","","Completed","2020-02-03","No","No","No","Internal"]
[null,null,null,null,10631,"23_14/02/2020 4:30:09 PM","2020-01-25","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Area below the cargo pumps need to be scraped/ cleaned and painted","Cargo Mach.","Cargo / Ballast Systems","Behaviour Based","8.51","Low","","","Area below the cargo pumps scraped, cleaned and painted","2020-02-05","","Completed","2020-02-03","No","No","No","Internal"]
[null,null,null,null,10632,"23_14/02/2020 4:32:02 PM","2020-01-25","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Oil sighted in AUS sealing tank sight glass","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.45","High","","","AUS tank sight glass cleaned & put back in position","2020-01-27","","Completed","2020-01-26","No","No","No","Internal"]
[null,null,null,null,10633,"23_14/02/2020 4:33:43 PM","2020-01-25","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Pump room damper wire out of pulley and not aligned.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","5.19","Medium","","","Pump room damper wire adjusted, function test carried out. Working in order.","2020-01-27","","Completed","2020-02-03","No","No","No","Internal"]
[null,null,null,null,10634,"23_14/02/2020 4:37:05 PM","2020-01-25","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Some oil spill gear in forecastle store kept on stbd side to be moved to miship store. Clear the unwanted old ropes, ladders, etc at Singapore ","Miscellaneous","General Appearance","Behaviour Based","11.12","Low","","","Oil spill gear shifted from forecastle store. Old mooring ropes and pilot ladder offlanded at Singapore","2020-02-07","","Completed","2020-02-07","No","No","No","Internal"]
[null,null,null,null,10635,"23_14/02/2020 4:42:46 PM","2020-01-25","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Hydroblaster maintenance to be done prior to the paint supply at Singapore and also check the condition of slury and grit blaster. All the machines to be put in use once the paints is received at Singapore","Miscellaneous","General Appearance","Behaviour Based","","","","","Hydroblaster maintenance done prior to the paint supply at Singapore and also checked the condition of slury and grit blaster. All the machines put in use. ","2020-02-10","","Completed","2020-01-27","No","No","No","Internal"]
[null,null,null,null,10636,"23_14/02/2020 5:03:31 PM","2020-01-25","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Fire doors in stairway, very slow to close. Need to be adjusted.","Accommodation","Safety / LSA / FFA","Equipment Related","5.1","Very High","","","Door closure of fire doors adjusted","2020-02-24","","Completed","2020-02-05","No","No","No","Internal"]
[null,null,null,null,10637,"23_14/02/2020 4:45:47 PM","2020-01-25","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Bridge AC filter very dirty/ should be cleaned as required or min once in a month","Miscellaneous","General Appearance","Human Error","10.32","Very High","","","Bridge AC filter cleaned.","2020-02-03","","Completed","2020-02-14","No","No","No","Internal"]
[null,null,null,null,11635,"23_30/04/2020 7:58:09 PM","2020-01-30","Observation","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","Bunker line drain valve not fitted with drain caps.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","6.8","High","","","Drain caps fabricated and fit on bunker line drain valve.","2020-02-10","","Completed","2020-02-15","No","No","No","External"]
[null,null,null,null,10878,"23_26/03/2020 3:01:04 PM","2020-02-28","Observation","Ship Staff","Ship Staff Insp.","No.1 Ballast eductor suction gauge inoperational.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.22","Very High","","","Requisition raised and replaced all in order.","2020-03-31","DHAW205001","Completed","2020-07-14","No","No","No","Internal"]
[null,null,null,null,10881,"23_26/03/2020 2:58:03 PM","2020-02-28","Observation","Ship Staff","Ship Staff Insp.","Both Ballast pumps revs cannot be controlled from CCR.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.18","High","","","Governor junction box opened and inspected. Voltage meter from CCR to governor motor checked & voltage noted 23.5V, found Governor responding.","2020-03-31","","Completed","2020-04-14","No","No","No","Internal","revert with troubleshooting and vessel requirement"]
[null,null,null,null,10879,"23_26/03/2020 3:03:23 PM","2020-03-02","Observation","Ship Staff","Ship Staff Insp.","Hand rail at Stbd. side manifold found heavily corroded.","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.6","Medium","","","Hand rail de-rusted and painted.","2020-04-27","","Completed","2020-04-30","No","No","No","Internal","complete and close out as per target date"]
[null,null,null,null,10880,"23_26/03/2020 3:06:33 PM","2020-03-05","Observation","Ship Staff","Ship Staff Insp.","Heavy rust spots on main deck forwad of Stbd. manifold.","Miscellaneous","General Appearance","Equipment Related","11.3","Medium","","","Hydroblasting and painting carried out.","2020-04-08","","Completed","2020-04-14","No","No","No","Internal"]
[null,null,null,null,9509,"23_08/01/2020 7:18:57 PM","2020-03-07","Defect","Ship Staff","Ship Staff Insp.","Atmospheric condenser cooling sea water inlet line leak after the sea water inlet valve.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Sea water inlet line to atmospheric condenser to be renewed. temporary repair using clamp in place.","2020-08-10","New Fabricated Sea water inlet line fitted in place with new valve.","Completed","2020-06-25","No","No","No","Internal","SW pipe is renewed , kindly close out the job."]
[null,null,null,null,10882,"23_29/03/2020 10:43:26 AM","2020-03-10","Observation","Ship Staff","Ship Staff Insp.","Travelling Jib crane mono rail cable damaged.","Deck - Machinery","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Mono rail cable renewed.","2020-04-20","","Completed","2020-04-29","No","No","No","Internal","kindly complete on priority and revert"]
[null,null,null,null,10883,"23_29/03/2020 10:46:07 AM","2020-03-11","Defect","Ship Staff","Ship Staff Insp.","Main engine air cooler no.1 sea water inlet/outlet pipe corroded.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Inlet and outlet pipe to be renewed once received fabricated pipe from shore workshop.","2020-08-30","","Completed","2020-09-26","No","No","No","Internal","material supplied; kindly revert with update and plans for close out"]
[null,null,null,null,10884,"23_29/03/2020 10:49:54 AM","2020-03-12","Observation","Ship Staff","Ship Staff Insp.","Sewage flushing line corroded and holed.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Pipeline renewed and the valve to sewage flushing line from sw service line was not holding, same renewed. ","2020-05-25","","Completed","2020-07-12","No","No","No","Internal","kindly complete and close out as per revised target date"]
[null,null,null,null,10885,"23_29/03/2020 10:51:30 AM","2020-03-12","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Water fountain coaming near engine room work shop corroded.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Coaming repaired by carrying out hotwork with office concurrence, job repoted in pal as unplanned activity","2020-04-30","","Completed","2020-07-08","No","No","No","Internal","kindly complete as per target date."]
[null,null,null,null,10894,"23_29/03/2020 10:48:26 AM","2020-03-12","Observation","Ship Staff","Ship Staff Insp.","COPT vaccum condensor pump no.2 sea water leak from shaft sleave.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","COPT vaccum condensor pumps o hauled , replaced with new sleeve","2020-04-12","","Completed","2020-03-17","No","No","No","Internal"]
[null,null,null,null,10893,"23_26/03/2020 3:08:58 PM","2020-03-14","Observation","Ship Staff","Ship Staff Insp.","3P bunker line inlet valve found leaking from gear box.","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.3","Medium","","","Leaking oil on deck cleaned. Gear box of 3P bunker line valve overhauled.","2020-03-14","","Completed","2020-03-14","No","No","No","Internal"]
[null,null,null,null,10886,"23_26/03/2020 3:17:57 PM","2020-03-15","Observation","Ship Staff","Ship Staff Insp.","Heater of dryer room in ship's laundry U-deck inoperational.","Accommodation","MLC Related","Equipment Related","11.14","Medium","","","Steam supply for the heater in dryer room checked and valve opened to ensure dryer works satisfactory.","2020-05-12","","Completed","2020-05-11","No","No","No","Internal","steam line repaired ; revert with the update on heater"]
[null,null,null,null,10887,"23_29/03/2020 10:53:05 AM","2020-03-15","Observation","Ship Staff","Ship Staff Insp.","AC compressor no.1 condesor inlet pipe holed.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Pipe fabricated and replaced.","2020-04-10","","Completed","2020-04-12","No","No","No","Internal","kindly make use of the two fitters an d close out on priority"]
[null,null,null,null,10888,"23_30/03/2020 10:39:11 AM","2020-03-19","Observation","Ship Staff","Ship Staff Insp.","Sapres inventory update","Miscellaneous","ISM Related","Equipment Related","10.12","Very High","","","All major spares updated including all pumps","2020-05-30","","Completed","2020-06-01","No","No","No","Internal","inventory in progress and expected completion end may 2020"]
[null,null,null,null,10889,"23_26/03/2020 3:21:04 PM","2020-03-20","Observation","Ship Staff","Ship Staff Insp.","Steam pipe passing through safety locker found leaking and accumulating lots of water.","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.12","Low","","","Steam pipe overhauled and leak arrested.","2020-03-31","","Completed","2020-04-05","No","No","No","Internal"]
[null,null,null,null,10890,"23_26/03/2020 3:22:51 PM","2020-03-20","Observation","Ship Staff","Ship Staff Insp.","Heavy rust spots on Cargo, Marpol and COW line.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","11.4","Very High","","","All cargo, marpol and COW line cross section at manifold de-rusted and paint.","2020-06-20","","Completed","2020-09-15","No","No","No","Internal","date extended, try to complete by target date.\nkindly close out on priority"]
[null,null,null,null,10891,"23_29/03/2020 10:55:36 AM","2020-03-24","Observation","Ship Staff","Ship Staff Insp.","24V battery malfunction.","Navigation - Others","Navigation","Equipment Related","10.32","Very High","","","New Battery installed. ","2020-04-08","","Completed","2020-04-05","No","No","No","Internal","upgrade service Po issued to Maretek and expected completion at Singapore on 04th april"]
[null,null,null,null,10892,"23_30/03/2020 10:35:31 AM","2020-03-26","Observation","Ship Staff","Ship Staff Insp.","Stbd. side manifold aft oxygen sensor of VECS system found malfunctioning.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.17","Low","","","Oxygen sensor for the VECS system replaced","2020-06-18","DHAW200119","Completed","2020-07-04","No","No","No","Internal","spares connected at Singapore - 30 june, kindly complete and close out."]
[null,null,null,null,11447,"23_15/04/2020 10:12:09 PM","2020-04-02","Observation","Ship Staff","Ship Staff Insp.","AC conder sea water inlet/outlet valve leaking.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Inlet & outlet valve renewed.","2020-04-15","","Completed","2020-04-13","No","No","No","Internal"]
[null,null,null,null,11448,"23_15/04/2020 5:37:33 PM","2020-04-07","Observation","Owner / Marine / Tech. Suptd.","Cargo Audit","Ship shore safety checklist point number 29 - Agreed tank venting system will be used answered as \"VESSEL DISCHARGING\"","Documentation","Cert. & Docu.","Human Error","5.9","Very High","","","Contents of Ship Shore safety checklist discussed with all deck officers. Remarks to be made for each sections discussed and understood by all officers.","2020-04-15","","Completed","2020-04-14","No","No","No","Internal"]
[null,null,null,null,11449,"23_15/04/2020 5:41:28 PM","2020-04-07","Observation","Owner / Marine / Tech. Suptd.","Bunkering Audit","Repetitive checks were not carried out as per bunker safety checklist \n\nIt states repetitive checks to be carried every 01 hour, check list completed at 1230 hrs but repetitive check commenced at 1400 hrs. \n\n\n\n","Documentation","Cert. & Docu.","Human Error","10.5","Low","","","Contents and importance of bunker checklist discussed with all officers and engineers.","2020-04-15","","Completed","2020-04-14","No","No","No","Internal"]
[null,null,null,null,11452,"23_15/04/2020 10:03:09 PM","2020-04-07","Observation","Ship Staff","Ship Staff Insp.","No.1 Main sea water pump discharge line elbow corroded and holed.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Discharge pipe elbow fabricated and fixed back.","2020-04-15","","Completed","2020-04-13","No","No","No","Internal"]
[null,null,null,null,11445,"23_15/04/2020 5:45:06 PM","2020-04-10","Observation","Ship Staff","Ship Staff Insp.","Dressor seals of Cargo, Marpol and COW line damaged at various locations.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","11.4","Very High","","","Dressor seals of Cargo, COW and Marpol line renewed.","2020-05-30","","Completed","2020-05-30","No","No","No","Internal","plan to complete after load port and carry our pr test prior to discharge port"]
[null,null,null,null,11450,"23_15/04/2020 10:05:00 PM","2020-04-10","Observation","Ship Staff","Ship Staff Insp.","No.2 DG L.T pump seal leaking.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","No. DG LT pump overhauled and seal replaced.","2020-04-15","","Completed","2020-04-14","No","No","No","Internal"]
[null,null,null,null,11451,"23_15/04/2020 10:13:55 PM","2020-04-10","Observation","Ship Staff","Ship Staff Insp.","DG 1 & 3 LT inlet valve not holding.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Inlet valves replaed with new ones.","2020-04-15","","Completed","2020-04-15","No","No","No","Internal"]
[null,null,null,null,11446,"23_15/04/2020 5:47:41 PM","2020-04-11","Observation","Ship Staff","Ship Staff Insp.","Hydraulic lines on deck for mooring winches and cranes thinning down and rusted at various locations","Deck - Pipe / Fittings","Mooring","Equipment Related","11.5","Medium","","","Hydraulic lines on deck for mooring winches no. 4, 6, 7, 8 and hose handling crane pipes renewed as required.","2020-08-31","","Completed","2020-08-27","No","No","No","Internal","spare pipe and material onboard- carry out planned replacement, work in progress and expected completion revised for end Aug"]
[null,null,null,null,11636,"23_30/04/2020 5:21:51 PM","2020-04-18","Observation","Ship Staff","Ship Staff Insp.","Runner control lever of Port hose handling crane malfunctioning.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.5","Very High","","","Control lever renewed with spare one. Port hose handling crane tried out and found to be working satisfactory.","2020-04-30","","Completed","2020-04-30","No","No","No","Internal"]
[null,null,null,null,11637,"23_30/04/2020 4:14:52 PM","2020-04-21","Observation","Ship Staff","Ship Staff Insp.","AUS gas drain valve to Slop Stbd. tank found very tight to operate.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.11","Medium","","","AUS drain valve to Slop Stbd overhauled and greased.","2020-05-05","","Completed","2020-04-30","No","No","No","Internal"]
[null,null,null,null,11638,"23_30/04/2020 3:44:29 PM","2020-04-22","Observation","Ship Staff","Ship Staff Insp.","Refer condesor no. 2 inlet pipe corroded.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","New pipe fabricated and put in place.","2020-04-30","","Completed","2020-04-28","No","No","No","Internal"]
[null,null,null,null,11639,"23_30/04/2020 3:48:54 PM","2020-04-23","Observation","Ship Staff","Ship Staff Insp.","DG no.2 oil max pump seal leaking.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Pump seal replaced.","2020-04-30","","Completed","2020-04-29","No","No","No","Internal"]
[null,null,null,null,11640,"23_30/04/2020 4:09:13 PM","2020-04-25","Observation","Ship Staff","Ship Staff Insp.","Port Side Lifeboat entrance hatch hinge broken.","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.28","Very High","","","Broken hinge removed and repaired. Entrance hatch hinge fixed back in location and found satisfactory.","2020-04-30","","Completed","2020-04-26","No","No","No","Internal"]
[null,null,null,null,11642,"23_30/04/2020 4:18:58 PM","2020-04-25","Observation","Ship Staff","Ship Staff Insp.","Both lifeboat lashing wires heavily rusted.","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.29","High","","","Lashing wire renewed, greased and covered with denso tape.","2020-04-30","","Completed","2020-04-28","No","No","No","Internal"]
[null,null,null,null,11641,"23_30/04/2020 3:47:07 PM","2020-04-26","Observation","Ship Staff","Ship Staff Insp.","Main engine unit no.4 Alpha Lubricator abnormal.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Alpha lubricator replaced with new spare.","2020-04-26","","Completed","2020-04-26","No","No","No","Internal"]
[null,null,null,null,11871,"23_17/05/2020 10:40:49 AM","2020-05-02","Observation","Ship Staff","Ship Staff Insp.","No.2 Refer AC condensor inlet pipe corroded and holed.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Pipe fabricated and replaced.","2020-05-10","","Completed","2020-05-03","No","No","No","Internal"]
[null,null,null,null,11872,"23_17/05/2020 10:42:34 AM","2020-05-03","Observation","Ship Staff","Ship Staff Insp.","Service pump no. 2 mechanical seal leak.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Pump overhauled and mechanical seal replaced.","2020-05-10","","Completed","2020-05-04","No","No","No","Internal"]
[null,null,null,null,11870,"23_17/05/2020 10:24:00 AM","2020-05-14","Observation","Ship Staff","Ship Staff Insp.","Stbd side manifold drain valve found leaking during cargo operation.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.11","Medium","","","Drain valve to 4S COT overhauled and inspected.","2020-05-20","","Completed","2020-05-20","No","No","No","Internal","complete the job and close out. check if replacement valves available in case if required"]
[null,null,null,null,12042,"23_27/05/2020 4:57:20 PM","2020-05-24","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Hydraulic leak was noted on the control block for the Main deck forward mooring winch MW1.","Deck - Mooring Machinery","Mooring","Equipment Related","9.14","Medium","","","Control block overhauled and seal renewed. Operation of mooring winch MW1 carried out no leaks found.","2020-06-07","","Completed","2020-05-27","No","No","No","Internal"]
[null,null,null,null,12043,"23_27/05/2020 5:00:25 PM","2020-05-24","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Some of the stickers / labels posted on the accommodation block were found faded","Accommodation","General Appearance","Equipment Related","11.13","Low","","","IMO stickers around accommodation renewed.","2020-06-07","","Completed","2020-05-29","No","No","No","Internal"]
[null,null,null,null,12044,"23_27/05/2020 5:04:26 PM","2020-05-24","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","For high level alarm, the identification board was found partly broken","Accommodation","General Appearance","Equipment Related","11.13","Low","","","High level identification board renewed.","2020-06-07","","Completed","2020-05-28","No","No","No","Internal"]
[null,null,null,null,12045,"23_27/05/2020 5:06:48 PM","2020-05-24","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","The upper cock for level gauge of the PV Breaker as well as the drain valve were found difficult to move. Also the water level in the PV Valve was not matching with the adjoining scale for the pressure","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.28","Medium","","","PV breaker level gauge valves made free and water level corrected.","2020-06-07","","Completed","2020-05-26","No","No","No","Internal"]
[null,null,null,null,12046,"23_27/05/2020 5:10:01 PM","2020-05-24","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Hydraulic leak from actuator of Valve COV-513, located forward of accommodation","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.11","Medium","","","Hydraulic connection of the actuator checked and made tight.","2020-06-07","","Completed","2020-05-29","No","No","No","Internal"]
[null,null,null,null,12047,"23_27/05/2020 5:19:44 PM","2020-05-24","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Bow visibility was not indicated in the Ballast Water exchange plan. ","Documentation","Cargo / Ballast Systems","Human Error","6.21","High","","","Bow visibility range included in the Ballast water exchange plan.","2020-06-07","","Completed","2020-05-30","No","No","No","Internal"]
[null,null,null,null,12048,"23_27/05/2020 5:22:12 PM","2020-05-24","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Procedures to be made for emergency Bilge pumping arrangement for pumproom. Basically what to do in case of pumproom flooding","Documentation","Cert. & Docu.","Human Error","8.47","Very High","","","Procedure for emergency bilge operation for pumproom flooding made and posted in CCR.","2020-06-07","","Completed","2020-05-25","No","No","No","Internal"]
[null,null,null,null,12049,"23_27/05/2020 5:25:04 PM","2020-05-24","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Monitoring of Navtex / EGC warnings should be more robust","Navigation - GMDSS & Communication","Navigation","Human Error","4.13","Very High","","","Company procedure being followed for monitoring of Navtex / EGC warnings.","2020-06-07","","Completed","2020-05-25","No","No","No","Internal"]
[null,null,null,null,12050,"23_27/05/2020 5:12:36 PM","2020-05-24","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","The eye for the embarkation ladder of the lifeboat was covered with denso tape. These are to be removed","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.47","Medium","","","Denso tapes on eye of the embarkation ladder removed.","2020-06-07","","Completed","2020-05-28","No","No","No","Internal"]
[null,null,null,null,12051,"23_27/05/2020 5:02:18 PM","2020-05-24","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Some of the vents were only marked with a number but not identified which space they were for","Accommodation","General Appearance","Equipment Related","11.13","Low","","","All vents stencilled and marked correctly.","2020-06-07","","Completed","2020-05-30","No","No","No","Internal"]
[null,null,null,null,6679,"23_20/11/2019 1:02:30 AM","2020-05-30","Defect","Ship Staff","Ship Staff Insp.","Provision crane slewing motor base is broken and is currently fixed in position by temporary arrangement.","Deck - Machinery","General Appearance","Equipment Related","8.5","Very High","","","Motor dismantled and maintenance is in progress","2021-01-31","DHAW200079","Completed","2020-12-27","No","No","No","Internal","Permanent repairs carried out and crane load tested satisfactory.\nalso complete spare onboard"]
[null,null,null,null,13013,"23_08/06/2020 5:38:44 PM","2020-06-02","Observation","Ship Staff","Ship Staff Insp.","Stbd side Aft Vapor line pressure gauge found faulty.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.61","Medium","","","Pressure gauge renewed.","2020-06-15","","Completed","2020-06-30","No","No","No","Internal"]
[null,null,null,null,13009,"23_08/06/2020 5:41:24 PM","2020-06-08","Observation","Ship Staff","Ship Staff Insp.","Vent valve on bunker line found without drain cap.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","6.8","High","","","Vent valve dismanteled from bunker line, brought to workshop and drain cap fabricated.","2020-06-15","","Completed","2020-07-10","No","No","No","Internal","kindly complete as planned and close out"]
[null,null,null,null,13011,"23_30/06/2020 1:27:25 PM","2020-06-24","Observation","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","Air leakage was found from the regulating valve of the air system in the starboard lifeboat at the time of inspection","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.29","High","","","Damaged part replaced with new received in Singapore","2020-07-25","","Completed","2020-07-28","No","No","No","External","spares awaiting supply, ready at forwarders"]
[null,null,null,null,13014,"23_30/06/2020 1:30:58 PM","2020-06-24","Observation","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","The dog ear of door of the battery store outside of the bridge was wasted due to corrosion and the door couldn't be locked if needed\t","Miscellaneous","Structural Condn. / WT integrity ","Equipment Related","11.6","Medium","","","Door shifted to engine room for welding and fabrication works carried out.","2020-07-24","","Completed","2020-06-28","No","No","No","External"]
[null,null,null,null,13015,"23_30/06/2020 1:19:26 PM","2020-06-24","Observation","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","Randomly checked the ballast water record book, it was found few times of ballast water taking on the open seas from Mar 2020, however the depth of the water was not recorded at the time of ballasting operation\t","Documentation","Cert. & Docu.","Human Error","2.13","Low","","","Training implemented by master to make correct entries in Ballast water record book","2020-07-25","","Completed","2020-06-27","No","No","No","External"]
[null,null,null,null,13010,"23_06/07/2020 9:19:20 PM","2020-06-30","Defect","Ship Staff","Ship Staff Insp.","Fresh watertank outlet valve not holding.","Hull & Tanks","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","fresh water tank outlet valve renewed.valve tested and found holding with no leaks.","2020-08-20","","Completed","2020-10-27","No","No","No","Internal","kindly complete as planned and close out. The tank was empty  ; kindly confirm if the job is completed."]
[null,null,null,null,13012,"23_06/07/2020 9:36:00 PM","2020-07-06","Observation","Ship Staff","Ship Staff Insp.","Air line iwo of 4C COT found leaking","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.4","Very High","","","Leakage rectified.","2020-07-20","","Completed","2020-07-18","No","No","No","Internal","complete as planned and close out"]
[null,null,null,null,13181,"23_16/07/2020 2:12:04 AM","2020-07-15","Defect","Ship Staff","Ship Staff Insp.","AE Fuel Oil Duplex filter change over cock stuck on one side","E/R - Air Comp.,E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","AE fuel duplex filter eased up.Now working satisfactory.","2020-08-27","","Completed","2020-12-16","No","No","No","Internal","please mention RO number in the PO reference. FYI Po is processed and will be connected once ready."]
[null,null,null,null,13180,"23_18/07/2020 11:07:06 PM","2020-07-18","Breakdown","Ship Staff","Ship Staff Insp.","3P IG Branch valve gear cover found broken during greasing","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.3","Very High","","","Gear cover renewed with the old spare valve cover","2020-07-25","","Completed","2020-07-22","No","No","No","Internal","kindly complete and close out as per planned date"]
[null,null,null,null,13473,"23_03/08/2020 1:28:59 PM","2020-07-25","Defect","Ship Staff","Ship Staff Insp.","FW hydrophore no.1 pump pressure switch defective, pump not cutting in","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.37","Medium","","","pressure switch renewed with new one. same tested and found working satisfactory.","2021-09-19","DHAW200165","Completed","2020-11-12","No","No","No","Internal","spares processed for supply"]
[null,null,null,null,13474,"23_03/08/2020 1:35:25 PM","2020-07-30","Defect","Ship Staff","Ship Staff Insp.","Ejector pump & IG seal water pump frame cracked","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.31","Very High","","","New pump fitted","2020-12-10","DHAW200175","Completed","2020-12-10","No","No","No","Internal","spare processed, follow up with purchase. close out the job on receipt of spares"]
[null,null,null,null,9191,"23_13/12/2019 11:20:44 PM","2020-07-31","Defect","Ship Staff","Ship Staff Insp.","#1 Fan shaft damaged which was built up and polished, bearings renewed and fitted back, now the blower is in operation but the bearing is running with slight high temperature compared to other blower. Vessel have received a spare shaft and bearings and kept in AC room. Plan to renew shaft when ship in cold weather","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Shaft and bearings renewed,tried out,found no abnormalities,bearing temperatures found normal.No abnormal noise or vibration found.","2021-01-31","","Completed","2021-01-15","No","No","No","Internal","plan to complete in China before or after port operations and revert upon completion. \n18th Jan: Please update status. No operational issues. kindly close out the job as long over due"]
[null,null,null,null,13475,"23_16/08/2020 7:34:07 PM","2020-08-04","Observation","Ship Staff","Ship Staff Insp.","Numerous deck pipelines U-Clamps and bolts found in rusty and wasted condition.","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.5","Medium","","","Renewal and derusting completed.","2021-01-25","","Completed","2021-01-01","No","No","No","Internal","Raise RO for small clamps; replace them. date revised to end JAn. work in progress"]
[null,null,null,null,13476,"23_16/08/2020 7:38:42 PM","2020-08-13","Observation","Ship Staff","Ship Staff Insp.","Spool piece of Sludge transfer pipe from engine to Slop S COT found rusted.","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.4","Very High","","","Maintenance carried out.","2020-08-20","","Completed","2020-09-15","No","No","No","Internal","kindly complete as planned and close out"]
[null,null,null,null,13477,"23_16/08/2020 7:48:35 PM","2020-08-15","Observation","Ship Staff","Ship Staff Insp.","Deck penetration pipes of hydraulic mooring winch 7 and 8 has wornout as per thicknees measurement and visual Inspection","Deck - Mooring Machinery","Mooring","Equipment Related","9.14","Medium","","","Renewed","2020-08-29","","Completed","2020-08-27","No","No","No","Internal","kindly complete as planned."]
[null,null,null,null,13951,"23_15/09/2020 9:27:45 PM","2020-09-15","Observation","Ship Staff","Ship Staff Insp.","Area between 5C to 4C COT various pipes need to be de-rusted and painting.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","11.4","Very High","","","Planned in upcoming maintenance","2020-12-15","","Completed","2020-11-23","No","No","No","Internal","to be completed as planned and close out"]
[null,null,null,null,14147,"23_03/10/2020 9:30:44 AM","2020-09-17","Defect","Ship Staff","Ship Staff Insp.","2C IG valve leaking","Inert Gas","Cargo / Ballast Systems","Equipment Related","8.31","High","","","Replaced IG v/v OF 2C","2021-01-31","DHAW200205","Completed","2021-01-06","No","No","No","Internal","spare connected; complete the job and close out"]
[null,null,null,null,14145,"23_03/10/2020 8:51:12 AM","2020-09-22","Defect","Ship Staff","Ship Staff Insp.","During Cargo operation, it was observed that No 3 Deck Cargo line X-over COV 509 could not be operated.Valve Operation : Hydraulic operated from main deck box no 6. Knob of the Valve operating lever was found stuck","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.21","High","","","Rectified, tested and found operational","2020-10-10","","Completed","2020-10-02","No","No","No","Internal","complete and close out as planned"]
[null,null,null,null,14146,"23_03/10/2020 8:53:25 AM","2020-09-27","Observation","Ship Staff","Ship Staff Insp.","Bridge wings Security light/Gangway lights found stuck and not movable, due to which gangway cannot be properly illuminated during personnel boarding","Miscellaneous","General Appearance","Equipment Related","5.47","Medium","","","Gangway lights lubricated and tested found operational","2020-10-10","","Completed","2020-10-04","No","No","No","Internal","complete and close out as planned"]
[null,null,null,null,16724,"23_04/01/2021 8:43:02 PM","2020-10-08","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","EGCS record book not updated ","Documentation","MARPOL Related","Human Error","10.11","Medium","","","Record book updated ","2020-11-04","","Completed","2020-10-30","No","No","No","Internal"]
[null,null,null,null,14281,"23_12/10/2020 11:00:34 AM","2020-10-08","Observation","Ship Staff","Ship Staff Insp.","No 2 Foam Monitor valve found leaking\t\t","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.38","High","","","Requisition raised and received, Foam monitor v/v replaced and tested no leaks observed.","2020-10-14","","Completed","2020-11-23","No","No","No","Internal"]
[null,null,null,null,15416,"23_23/11/2020 3:48:01 AM","2020-10-09","Defect","Ship Staff","Ship Staff Insp.","All Winches crossover hydraulic pipe found wasted and need to be replaced with new hydraulic pipe received.","Deck - Mooring Machinery","Mooring","External Factors","9.14","Medium","","","All Winches crossover hydraulic pipe replaced with new pipe. tested and found no leaks.","2020-11-23","","Completed","2020-11-22","No","No","No","Internal"]
[null,null,null,null,16719,"23_04/01/2021 8:49:15 PM","2020-10-09","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Duty engineer signature missing at few pages in engine room log book.","Documentation","ISM Related","Inappropriate Procedure","10.5","Low","","","Duty engineer signed immediately","2020-10-10","","Completed","2020-10-09","No","No","No","Internal"]
[null,null,null,null,16720,"23_04/01/2021 8:56:17 PM","2020-10-09","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Log entry not made for bunkering operation at Fujairah","Documentation","MARPOL Related","Inappropriate Procedure","10.5","Low","","","Log entry made for bunkering operation ","2020-10-16","","Completed","2020-10-11","No","No","No","Internal"]
[null,null,null,null,16721,"23_04/01/2021 9:01:08 PM","2020-10-09","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Engine room bell book few entries missing.Additional entries such as ME turned on turning gear,dg taken on load etc.missing","Documentation","ISM Related","Inappropriate Procedure","10.5","Low","","","all entries made and all engineers briefed.","2020-10-11","","Completed","2020-10-10","No","No","No","Internal"]
[null,null,null,null,14282,"23_12/10/2020 11:55:42 AM","2020-10-09","Defect","Ship Staff","Ship Staff Insp.","No 2 DG fuel oil pressure guage defective","E/R - Aux. Engine","Eng. / Strg. Comp.","Behaviour Based","10.32","Very High","","","No 2 DG fuel oil  pressure guage renewed with new one ,reading showing satisfactory.","2020-10-09","","Completed","2020-11-13","No","No","No","Internal","complete as planned"]
[null,null,null,null,16722,"23_04/01/2021 9:09:53 PM","2020-10-10","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","3/E and 4/E not maintaining daily workdone book.All engineers to maintain daily workdone book and a maintenance history book of their respective machinery.","Documentation","ISM Related","Inappropriate Procedure","10.5","Low","","","3/E and 4/E briefed and daily workdone book and machinery maintenance history book maintained ","2020-10-12","","Completed","2020-10-12","No","No","No","Internal"]
[null,null,null,null,16723,"23_04/01/2021 9:19:30 PM","2020-10-10","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Boiler water test log-qty of chemical dosed does not mention in the report ","Documentation","ISM Related","Inappropriate Procedure","","","","","Quantity of chemical mentioned in boiler log","2020-10-25","","Completed","2020-10-20","No","No","No","Internal"]
[null,null,null,null,16725,"23_04/01/2021 9:25:48 PM","2020-10-10","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","DG performance-Doctor report not attatched.","Documentation","ISM Related","Inappropriate Procedure","10.12","Very High","","","Doctor report attatched ","2020-10-20","","Completed","2020-10-17","No","No","No","Internal"]
[null,null,null,null,16726,"23_04/01/2021 9:30:48 PM","2020-10-10","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","E/R tanktop needs cosmetic upgradation ","Miscellaneous","General Appearance","Equipment Related","10.29","Medium","","","Cleaning and painting of tanktop done","2020-11-09","","Completed","2020-11-01","No","No","No","Internal"]
[null,null,null,null,16727,"23_04/01/2021 9:34:16 PM","2020-10-10","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","E/R bilge well stbd has oil content .Oil to be scummed off and source of leak to be rectified.","Miscellaneous","General Appearance","Equipment Related","10.29","Medium","","","Oil removed by absorbent pads and source of leak rectified.","2020-10-20","","Completed","2020-10-18","No","No","No","Internal"]
[null,null,null,null,16729,"23_04/01/2021 9:12:45 PM","2020-10-10","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","2/E workdone hand written not updated","Documentation","ISM Related","Inappropriate Procedure","10.5","Low","","","Daily workdone record updated","2020-10-12","","Completed","2020-10-12","No","No","No","Internal"]
[null,null,null,null,14283,"23_12/10/2020 12:14:53 PM","2020-10-10","Defect","Ship Staff","Ship Staff Insp.","Main engine air cooler No2 Manometer defective","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Tubes and associated pipes cleaned.","2020-10-10","","Completed","2020-12-17","No","No","No","Internal","complete as planned"]
[null,null,null,null,16728,"23_04/01/2021 10:24:33 PM","2020-10-11","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","F.W.G. production low temperature difference of evaporator inlet/outlet is 5 deg.Need chemical cleaning/descaling.Maker recommended temperature diff of 12 deg","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Fresh water generator chemical cleaning done .Production increased.","2020-10-21","","Completed","2020-10-19","No","No","No","Internal"]
[null,null,null,null,16730,"23_04/01/2021 10:32:02 PM","2020-10-11","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Engine room dust accumulated on floor/bulkheads/pipelines in engine room.To be thoroughly cleaned and to be maintained in clean condition hence forth.Ratings to be assigned responsibility of platforms to maintain in clean condition.ER floors to be mopped atleast once in a week.","Miscellaneous","General Appearance","Equipment Related","10.29","Medium","","","Engine room floor/bulkheads and pipelines cleaned.Ratings assigned responsibility of platforms.","2020-10-20","","Completed","2020-10-19","No","No","No","Internal"]
[null,null,null,null,16731,"23_04/01/2021 10:36:11 PM","2020-10-11","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Fire and bilge pump suction valve not holding .To be renewed","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.31","Very High","","","Renewed with spare new valve ","2020-11-18","","Completed","2020-11-13","No","No","No","Internal"]
[null,null,null,null,16732,"23_04/01/2021 10:42:18 PM","2020-10-11","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","E/R workshop need cosmetic upgradation-welding area to be marked.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Workshop painted and welding area marked and curtain used.","2020-11-10","","Completed","2020-11-04","No","No","No","Internal"]
[null,null,null,null,16733,"23_04/01/2021 10:45:43 PM","2020-10-11","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Welding curtain need to be renewed","Miscellaneous","General Appearance","Equipment Related","10.29","Medium","","","Welding curtain renewed ","2020-11-09","","Completed","2020-11-04","No","No","No","Internal"]
[null,null,null,null,14284,"23_12/10/2020 12:26:44 PM","2020-10-11","Defect","Ship Staff","Ship Staff Insp.","Boiler water circulating pump no 2 leakage from gland.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","pump overhauled,after installing same all found working satisfactory.","2020-10-11","","Completed","2020-11-07","No","No","No","Internal","complete overhaul as planned and close out"]
[null,null,null,null,14285,"23_12/10/2020 12:37:15 PM","2020-10-11","Observation","Ship Staff","Ship Staff Insp.","Salt deposition & Oil stains on E/R tank top.","Miscellaneous","General Appearance","Behaviour Based","10.25","Very High","","","Descaling,washing & painting  carried out.","2020-11-11","","Completed","2020-11-01","No","No","No","Internal","complete as planned"]
[null,null,null,null,14286,"23_13/10/2020 6:51:46 PM","2020-10-11","Defect","Ship Staff","Ship Staff Insp.","Main engine no-2 , 5 & 6 units slight exhaust leakage between exhaust outlet & manifold .","E/R - Main Engine","Eng. / Strg. Comp.","External Factors","10.32","Very High","","","Leakage rectified ,now no leak from no 2,5 & 6 units","2020-11-11","","Completed","2020-10-20","No","No","No","Internal"]
[null,null,null,null,16699,"23_04/01/2021 11:03:58 PM","2020-10-12","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Engine log printer not operational","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Log printer to be renewed","2021-01-30","DHAW210004","Completed","2021-01-20","No","No","No","Internal","AMS printer is functional .\nLog printer , NOON DLOG BOOK is maintained and there is no requirement for printed log."]
[null,null,null,null,16734,"23_04/01/2021 10:49:46 PM","2020-10-12","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","E.C.R. floor dirty.Need cleaning and waxing.E.c.r. floor to be mopped everyday with out fail","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","E.C.R .floor waxed.Floor mopped and maintained on a daily basis.","2020-10-14","","Completed","2020-10-14","No","No","No","Internal"]
[null,null,null,null,16735,"23_04/01/2021 10:57:30 PM","2020-10-12","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Corrocoat paint stowed in E.C.R.Paint to be stowed in plywood box with holes.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","5.46","Medium","","","Plywood box made with holes and paint stowed in it.","2020-10-27","","Completed","2020-10-25","No","No","No","Internal"]
[null,null,null,null,16736,"23_04/01/2021 11:09:25 PM","2020-10-12","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","E.C.R. A/C condenser cover left open.Condenser cover to be put back the tray to be cleaned and painted.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Human Error","10.32","Very High","","","Condenser cover fitted back in position,tray cleaned and painted.","2020-11-11","","Completed","2020-11-01","No","No","No","Internal"]
[null,null,null,null,14287,"23_15/10/2020 10:58:34 PM","2020-10-12","Defect","Ship Staff","Ship Staff Insp.","No 3 generator fuel oil inlet valve hair line crack from valve bonnet.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","NO 3 GE FUEL OIL INLET VALVE REPLACED WITH NEW ONE ,GE TESTED WORKING SATISFACTORY.","2020-11-30","","Completed","2020-11-13","No","No","No","Internal","plan and complete at suitable location .on priority"]
[null,null,null,null,16737,"23_04/01/2021 11:17:42 PM","2020-10-13","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","CCR IG panel few indication lamps not working.","Elect. Mach. & Equip.","Cargo / Ballast Systems","Equipment Related","8.25","Very High","","","Indication lamps renewed","2020-10-18","","Completed","2020-10-17","No","No","No","Internal"]
[null,null,null,null,16738,"23_04/01/2021 11:24:23 PM","2020-10-13","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Main engine unit no:2,5&6 has exhaust gas leak from exhaust bellow","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Leakage rectified by tightening of flange bolts","2020-11-12","","Completed","2020-10-20","No","No","No","Internal"]
[null,null,null,null,16739,"23_04/01/2021 11:35:13 PM","2020-10-13","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Both main engine air coolers end covers have rust marks .Need derusting and painting.","E/R - Main Engine","General Appearance","Equipment Related","10.31","Very High","","","Both end covers cleaned,derusted and painted ","2020-11-09","","Completed","2020-11-04","No","No","No","Internal"]
[null,null,null,null,16745,"23_04/01/2021 11:28:11 PM","2020-10-13","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","M/E unit no.1 Aft fuel valve has leakage from H.P. pipe.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","H.P. pipes o-rings renewed.","2020-11-12","","Completed","2020-11-04","No","No","No","Internal"]
[null,null,null,null,16740,"23_04/01/2021 11:40:07 PM","2020-10-14","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","M.G.P.S.rust marks on top cover and bolts ","E/R - Aux. Mach.","General Appearance","Equipment Related","10.31","Very High","","","Derusting and painting done.","2020-11-04","","Completed","2020-11-04","No","No","No","Internal"]
[null,null,null,null,16741,"23_04/01/2021 11:45:54 PM","2020-10-14","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Antisplash tapes to be pit on ME fuel oil HP pipes.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.19","Very High","","","Anti splash tapes put on main engine fuel oil HP pipes.","2020-10-28","","Completed","2020-10-25","No","No","No","Internal"]
[null,null,null,null,16742,"23_04/01/2021 11:48:32 PM","2020-10-14","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","No:2 DG fuel oil pressure gauge not functioning","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Pressure gauge renewed.","2020-10-24","","Completed","2020-10-23","No","No","No","Internal"]
[null,null,null,null,16743,"23_04/01/2021 11:54:20 PM","2020-10-14","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","No:2 D/G alternator bearing giving high temperature alarm.Portable fan used to cool down.Maker to be consulted to sort out the issue.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Maker consulted and the quantity of oil reduced in the bearing.","2020-12-07","","Completed","2020-11-15","No","No","No","Internal"]
[null,null,null,null,16744,"23_04/01/2021 11:59:38 PM","2020-10-15","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","No:2 DG oil leakage in tray to be rectified","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.19","Very High","","","Oil leakage from lubricating oil pump outlet line  rectified","2020-10-25","","Completed","2020-10-24","No","No","No","Internal"]
[null,null,null,null,16746,"23_05/01/2021 12:05:35 AM","2020-10-15","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Steam leak behind hotwell","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.31","Very High","","","Steam leakage rectified from return line near hotwell.","2020-10-25","","Completed","2020-10-20","No","No","No","Internal"]
[null,null,null,null,16747,"23_05/01/2021 12:29:01 AM","2020-10-15","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Vacuum condenser is operated at -35% vacuum.Source of leak to be identified,Vacuum should be improved.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Steam ejector condenser cleaned,outlet valve to air ejector condenser renewed.Valve glands tightened.Gland steam pressure adjusted.Copt condenser cleaned. ","2020-11-04","","Completed","2020-12-05","No","No","No","Internal"]
[null,null,null,null,16748,"23_05/01/2021 12:34:41 AM","2020-10-15","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","AUS vacuum pump grease below red line ","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Grease topped up ","2020-10-23","","Completed","2020-10-22","No","No","No","Internal"]
[null,null,null,null,14288,"23_15/10/2020 11:02:13 PM","2020-10-15","Defect","Ship Staff","Ship Staff Insp.","window wiper port centre ( No 2 ) not working .","Navigation - Others","Navigation","Equipment Related","12.1","High","","","WINDOW WIPER REPAIRED ,BELT ASSEMBLY AND ROLLERS RENEWED,SAME TESTED AND FOUND WORKING SATISFACTORY.","2020-11-15","","Completed","2020-10-17","No","No","No","Internal","please check the spares and ROB. complete as planned"]
[null,null,null,null,14289,"23_15/10/2020 11:08:12 PM","2020-10-15","Defect","Ship Staff","Ship Staff Insp.","Fire & bilge pump suction filter water leakage","E/R - Pipes/ valves & fittings,E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","5.35","Medium","","","SUCTION VALVE RENEWED BY ISOLATING BOTH SEA CHEST SUCTION.NO WATER LEAKAGE FROM FILTER ","2020-11-30","","Completed","2020-11-15","No","No","No","Internal","spare valves on ship; replace and complete as planned"]
[null,null,null,null,16749,"23_05/01/2021 12:39:56 AM","2020-10-16","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ODME sample pump bulkhead seal oil less.Oil to be filled up ","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","6.13","Low","","","Oil filled up and leakage rectified ","2020-10-21","","Completed","2020-10-20","No","No","No","Internal"]
[null,null,null,null,16750,"23_05/01/2021 12:44:58 AM","2020-10-16","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Spares parts box lying on deck unsecured,spares to be shifted.","Miscellaneous","General Appearance","Behaviour Based","4.4","High","","","Spare parts box shifted to spare parts store.","2020-10-21","","Completed","2020-10-19","No","No","No","Internal"]
[null,null,null,null,16751,"23_05/01/2021 12:55:26 AM","2020-10-16","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Deck foam pump coupling guard left open ","LSA / FFA","Emgcy. Systems","Equipment Related","5.35","Medium","","","Coupling guard fitted.","2020-10-21","","Completed","2020-10-19","No","No","No","Internal"]
[null,null,null,null,16752,"23_05/01/2021 1:06:21 AM","2020-10-16","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","AC room needs cosmetic upgrade.Refrigerant gas bottles and n2 gas bottles to be secured on bulkhead with proper clamps .Unwanted used spares to be scrapped and racks to be cleaned and painted ","Miscellaneous","General Appearance","Human Error","10.29","Medium","","","Ac blower room cleaned and painted,gas bottles secured with clamps,used spares put in garbage,racks painted.","2020-11-15","","Completed","2020-11-04","No","No","No","Internal"]
[null,null,null,null,16700,"23_05/01/2021 2:40:47 AM","2020-10-17","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","2 nos R-22 bottles lying in steering gear room .These bottles to be offlanded as R22 are not used anymore.","Miscellaneous","Eng. / Strg. Comp.","Industry Issue","10.32","Very High","","","R-22 bottles to be stowed at different location","2021-03-09","","Completed","2021-01-18","No","No","No","Internal","bottle moved to steering gear flat"]
[null,null,null,null,16753,"23_05/01/2021 1:10:51 AM","2020-10-17","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","NO:2 Main air compressor first stage pressure low .To be investigated.","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Auto drain valve found leaking same o'hauled and fitted back.","2020-11-04","","Completed","2020-11-04","No","No","No","Internal"]
[null,null,null,null,16754,"23_05/01/2021 1:15:16 AM","2020-10-17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Incinerator sludge tank has clear signs of overflow on laggings.Tank laggings to be painted with silver colour paint.","E/R - Aux. Mach.","General Appearance","Human Error","10.32","Very High","","","Laggings on incinerator tank cleaned and painted ","2020-11-11","","Completed","2020-11-04","No","No","No","Internal"]
[null,null,null,null,16755,"23_05/01/2021 1:24:18 AM","2020-10-17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Garbage oily rags stored on floor near incinerator in plastic bags.No garbage should be stored outside metal containers.All garbage should be shifted to garbage locker and to be transferred near incinerator during garbage burning.","Miscellaneous","Eng. / Strg. Comp.","Human Error","6.2","High","","","Garbage stored in metal containers only.Excess garbage stored in garbage locker.","2020-10-19","","Completed","2020-10-19","No","No","No","Internal"]
[null,null,null,null,16756,"23_05/01/2021 2:44:50 AM","2020-10-17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Empty carton boxes lying in steering flat to be incinerated.","Miscellaneous","Eng. / Strg. Comp.","Human Error","6.2","High","","","Boxes incinerated ","2020-11-02","","Completed","2020-11-01","No","No","No","Internal"]
[null,null,null,null,16757,"23_05/01/2021 2:49:54 AM","2020-10-17","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","area of bilge alarm floats to be identified with yellow paint.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.3","Medium","","","bilge alarms area painted yellow","2020-10-17","","Completed","2020-11-03","No","No","No","Internal"]
[null,null,null,null,16758,"23_05/01/2021 2:55:10 AM","2020-10-17","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Empty chemical drums lying on bulkhead stringers to be removed and scrapped","Miscellaneous","Eng. / Strg. Comp.","Human Error","6.2","High","","","Removed and put in plastic garbage.Later to be  landed ashore.","2020-11-16","","Completed","2020-11-03","No","No","No","Internal"]
[null,null,null,null,16759,"23_05/01/2021 2:58:14 AM","2020-10-17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","  lL.O. pails stored on floor.All L.O. pails to be accommodated on racks","Miscellaneous","Eng. / Strg. Comp.","Human Error","10.29","Medium","","","All L.O. pails accommodated on racks ","2020-11-15","","Completed","2020-11-03","No","No","No","Internal"]
[null,null,null,null,16763,"23_05/01/2021 1:31:05 AM","2020-10-17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Spare parts lying on floor to be shifted to racks.","Miscellaneous","Eng. / Strg. Comp.","Human Error","10.12","Very High","","","Spares shifted to racks and arranged.","2020-11-02","","Completed","2020-11-01","No","No","No","Internal"]
[null,null,null,null,14730,"23_07/11/2020 10:21:15 AM","2020-10-17","Defect","Ship Staff","Ship Staff Insp.","HI HI LEVEL ALARM NO 1 STBD COT & 4 PORT COT NOT SHOWING CORRECT READING.","Elect. Mach. & Equip.","Cargo / Ballast Systems","Equipment Related","8.26","High","","","SPARES ORDERED ,SAME TO BE RENEWED AFTER GETTING SPARES.","2021-01-15","DHAW200217","Completed","2020-12-31","No","No","No","Internal","spares onboard. \n4P COT sensor replaced today. \ncomplete the job and close out"]
[null,null,null,null,16760,"23_05/01/2021 1:34:40 AM","2020-10-18","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Air pressure regulator pressure gauge for sewage treatment plant found faulty.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Pressure gauge renewed.","2020-10-25","","Completed","2020-10-24","No","No","No","Internal"]
[null,null,null,null,16761,"23_05/01/2021 1:38:01 AM","2020-10-18","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Sewage treatment plant tray to be cleaned and plant soap washed ","E/R - Aux. Mach.","General Appearance","Equipment Related","10.32","Very High","","","Plant soapwashed and tray cleaned.","2020-11-05","","Completed","2020-11-01","No","No","No","Internal"]
[null,null,null,null,16762,"23_05/01/2021 2:15:52 AM","2020-10-18","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Spare piston rings stowed on E/R 2nd deck forward-Lead padding to be given to prevent fretting.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Lead padding fitted on the area of resting of piston rings.","2020-10-28","","Completed","2020-10-26","No","No","No","Internal"]
[null,null,null,null,16764,"23_05/01/2021 3:01:15 AM","2020-10-18","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Exhaust manifold drain pot near No:1 boiler empty.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Human Error","10.32","Very High","","","Water filled in the drain pot and crew briefed to fill up water on a regular basis.","2020-10-20","","Completed","2020-10-20","No","No","No","Internal"]
[null,null,null,null,16765,"23_05/01/2021 3:10:36 AM","2020-10-18","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Engine room changing locker Paint near wash basin spoilt,area to be scrapped and painted.","Miscellaneous","General Appearance","Human Error","10.31","Very High","","","Engine room changing locker floor near wash basin scrapped and painted ","2020-11-08","","Completed","2020-11-01","No","No","No","Internal"]
[null,null,null,null,16766,"23_05/01/2021 3:17:58 AM","2020-10-18","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Spare parts box and calibration gas bottles lying in scrubber room to be secured properly.","Miscellaneous","Eng. / Strg. Comp.","Human Error","10.32","Very High","","","Spare parts boxes and gas bottles secured.","2020-10-21","","Completed","2020-10-20","No","No","No","Internal"]
[null,null,null,null,16773,"23_05/01/2021 3:13:54 AM","2020-10-18","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Scrubber room ventilation louvres rusted,need derusting and painting.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.31","Very High","","","Derusted and painted ","2020-12-18","","Completed","2020-12-15","No","No","No","Internal"]
[null,null,null,null,16701,"23_05/01/2021 2:19:15 AM","2020-10-19","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Spare part racks and spare part boxes to be numbered ","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.12","Very High","","","Numbering of racks and boxes completed.","2021-02-11","","Completed","2021-02-15","No","No","No","Internal"]
[null,null,null,null,16767,"23_05/01/2021 2:26:27 AM","2020-10-19","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Fire hose near E.G.B. not secured.","LSA / FFA","Eng. / Strg. Comp.","Human Error","5.34","Low","","","Fire hose rolled and secured.","2020-10-21","","Completed","2020-10-20","No","No","No","Internal"]
[null,null,null,null,16768,"23_05/01/2021 2:34:49 AM","2020-10-19","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","200 ltr L.O. drums found lying near L.O. tanks not secured by lashing.","Miscellaneous","Eng. / Strg. Comp.","Human Error","10.29","Medium","","","L.O. drums shifted to steering flat and secured by wire rope.","2020-10-24","","Completed","2020-10-23","No","No","No","Internal"]
[null,null,null,null,16769,"23_05/01/2021 3:28:19 AM","2020-10-19","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","7EX proof lights Diffusers  found to have cracks.Needs renewal ","Elect. Mach. & Equip.","Safety / LSA / FFA","Equipment Related","10.32","Very High","","","Requisition received at singapore,All diffusers renewed.","2021-01-20","","Completed","2021-01-01","No","No","No","Internal"]
[null,null,null,null,16702,"23_05/01/2021 3:33:00 AM","2020-10-20","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Spare parts inventory update in PAL to impriove.Spare parts location not updated -Spare boxes and racks to be numbered,and location to be fed for each spare parts ","Miscellaneous","Eng. / Strg. Comp.","Inappropriate Procedure","10.32","Very High","","","Inventory updated in PAL","2021-02-15","","Completed","2021-02-27","No","No","No","Internal"]
[null,null,null,null,16770,"23_05/01/2021 3:37:12 AM","2020-10-20","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","33 Job orders in P.M.S have not been triggered.","Miscellaneous","ISM Related","Human Error","10.12","Very High","","","Jobs triggerred ","2020-10-22","","Completed","2020-10-22","No","No","No","Internal"]
[null,null,null,null,16771,"23_05/01/2021 3:40:46 AM","2020-10-20","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","DG running hour reports ,governor o'haul of all three auxiliary engines showing overdue.If job was carried out at DD,Rhrs has to be updated,else job to be carried out.","Documentation","ISM Related","Human Error","10.32","Very High","","","O'haul done in dry dock,running hours updated.","2020-11-05","","Completed","2021-01-03","No","No","No","Internal"]
[null,null,null,null,14732,"23_07/11/2020 10:26:36 AM","2020-10-20","Defect","Ship Staff","Ship Staff Insp.","NO 2 HFO PURIFIER FEED PUMP OIL LEAKAGE FROM SHAFT GLAND PACKING.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","GLAND PACKING RENEWED.","2020-11-30","","Completed","2020-11-30","No","No","No","Internal"]
[null,null,null,null,16772,"23_05/01/2021 1:14:57 PM","2020-10-21","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Midship locker house keeping to improve. Arrange all items.","Miscellaneous","General Appearance","Human Error","10.29","Medium","","","All Items properly secured and cleaning carried out.","2020-11-05","","Completed","2020-11-03","No","No","No","Internal"]
[null,null,null,null,16774,"23_05/01/2021 1:17:38 PM","2020-10-21","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Hose handling crane rust marks noticed on weld joint of working platform to crane jib.","Deck - Machinery","General Appearance","External Factors","11.4","Very High","","","Derusting and painting carried out.","2020-11-05","","Completed","2020-11-03","No","No","No","Internal"]
[null,null,null,null,16775,"23_05/01/2021 1:21:30 PM","2020-10-21","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Stbd windlass hydraulic motor has hydraulic oil leak from the shaft seal","Deck - Mooring Machinery","Mooring","External Factors","9.14","Medium","","","Shaft seal of the hydraulic motor replaced with new seal. tested no leaks observed.","2020-11-05","","Completed","2020-11-01","No","No","No","Internal"]
[null,null,null,null,16776,"23_05/01/2021 1:43:06 PM","2020-10-21","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","6M inspection of Ballast tank 5S reported without actually doingit. Tank to be inspected and DNV report to be attached to Job","Hull & Tanks","Cargo / Ballast Systems","Human Error","2.9","Medium","","","Ballast tank 5S  inspection was carried out and DNV form was duly attached., JO no: DHAW026673/20","2020-10-31","","Completed","2020-10-25","No","No","No","Internal"]
[null,null,null,null,16777,"23_05/01/2021 1:46:28 PM","2020-10-21","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Officer laundry Washing machine used for boiler suit leaking","Miscellaneous","General Appearance","Equipment Related","11.16","Low","","","Requisition raised and received in Singapore on 10th Nov 2020 & replaced with leaking washing machine","2020-11-15","DHAW200227","Completed","2020-11-12","No","No","No","Internal"]
[null,null,null,null,16778,"23_05/01/2021 1:48:53 PM","2020-10-21","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Old ropes lying in steering flat room and forecastle deck to be scrapped","Miscellaneous","General Appearance","Equipment Related","6.2","High","","","Landed in Singapore on 23rd Dec 2020.","2020-12-31","","Completed","2020-12-23","No","No","No","Internal"]
[null,null,null,null,16779,"23_05/01/2021 1:55:50 PM","2020-10-21","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Gangway ladder Stbd steps need to be derusted and painted.","Miscellaneous","General Appearance","External Factors","5.47","Medium","","","Derusting and painting carried out.","2020-11-15","","Completed","2020-11-09","No","No","No","Internal"]
[null,null,null,null,16780,"23_05/01/2021 2:38:29 PM","2020-10-21","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Cockroach found in accommodation. Fumigation has to be carried out in accommodation.","Accommodation","MLC Related","Human Error","11.13","Low","","","Fumigation in accommodation carried out in Fujairah anchorage.","2020-12-23","","Completed","2020-11-30","No","No","No","Internal"]
[null,null,null,null,14733,"23_07/11/2020 10:29:11 AM","2020-10-21","Defect","Ship Staff","Ship Staff Insp.","CALORIFIER STEAM INLET PILE GASKET DAMAGED,HENCE STEAM IS LEAKING.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","GASKET RENEWED.","2020-11-30","","Completed","2020-12-14","No","No","No","Internal"]
[null,null,null,null,14745,"23_09/11/2020 12:18:44 AM","2020-10-31","Defect","Ship Staff","Ship Staff Insp.","ODME valve to slop (S) COV 513 found hydraulic oil leaking into the valve & over flowed on deck.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.11","Medium","","","valve hydraulic line isolated. Valve drain plug Opened & hydraulic oil drained. leaking shut side & seal renwed with new seal & found rubber seal was new but fit in wrong way. Fit in a correct way & box back. Valve operated & found no leaks in the valve.","2020-11-06","","Completed","2020-11-04","No","No","No","Internal"]
[null,null,null,null,14747,"23_09/11/2020 12:20:37 AM","2020-10-31","Defect","Ship Staff","Ship Staff Insp.","Valve COV 822 hydraulic oil leaking from the actuator open side.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.11","Medium","","","Actuator Seal on open side found damage, seal renewed.","2020-11-06","","Completed","2020-11-04","No","No","No","Internal"]
[null,null,null,null,16781,"23_05/01/2021 1:08:50 PM","2020-11-04","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","5C COT tank manhole cover need derusting and painting","Deck - Pipe / Fittings","General Appearance","External Factors","11.4","Very High","","","Derusting and painting carried out.","2020-11-06","","Completed","2020-11-04","No","No","No","Internal"]
[null,null,null,null,14734,"23_16/11/2020 12:35:09 AM","2020-11-07","Defect","Ship Staff","Nav Audit / Verification","BW-V823 Ballast discahrge v/v of WBP # 2, found pin hole water leaking during ballasting operation","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.21","High","","","V/v removed and cold work done, RO raised DHAW200247.","2020-12-14","DHAW200247","Completed","2020-11-15","No","No","No","Internal","valve will be processed on priority .\nreplace on receipt."]
[null,null,null,null,16703,"23_05/01/2021 2:00:07 PM","2020-11-11","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Mooring rope need renewal, as informed by C/O","Deck - Mooring Machinery,Miscellaneous","Mooring","External Factors","9.17","High","","","New Mooring wire  rope replacing M2 outward side. ","2021-03-04","","Completed","2021-03-01","No","No","No","Internal"]
[null,null,null,null,16706,"23_05/01/2021 1:35:15 PM","2020-11-11","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Hydroblaster not developing pressure.","Miscellaneous","General Appearance","Equipment Related","1.16","Low","","","Nozzles renewed in Apr 2021 after receipt of spare nozzles. The pressure now is 330 bar. Working pressure is 800 bars. Noted water leaking from the plunger tell tale hole, plunger seals leaking, RO raised.","2021-09-30","DHAW210225 raised","Completed","2021-08-24","No","No","No","Internal","equipment operational  with loss in pressure.\nmore spares on RO. \nequipment is operational hence closed out"]
[null,null,null,null,16782,"23_05/01/2021 12:45:23 PM","2020-11-11","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Heating steam lines and valves need derusting and painting","Deck - Pipe / Fittings","General Appearance","External Factors","8.15","High","","","Derusting and painting carried out.","2020-11-30","","Completed","2020-11-23","No","No","No","Internal"]
[null,null,null,null,16783,"23_05/01/2021 12:48:29 PM","2020-11-11","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Old wire need to be scrapped","Miscellaneous","Eng. / Strg. Comp.","Human Error","6.2","High","","","Scrap Landed in garbage at Singapore","2020-12-31","","Completed","2020-12-23","No","No","No","Internal"]
[null,null,null,null,14736,"23_11/11/2020 12:18:32 PM","2020-11-11","Defect","Ship Staff","Ship Staff Insp.","PORT BOILER GAUGE GLASS NOT SHOWING LEVEL.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Gauge glass o'hauled and packing renewed.","2020-11-30","","Completed","2020-12-16","No","No","No","Internal","to be completed on priority"]
[null,null,null,null,16784,"23_05/01/2021 12:51:16 PM","2020-11-11","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","IG line near Slop-S need to be derusted and painted","Deck - Pipe / Fittings","General Appearance","External Factors","8.23","Medium","","","Derusting and painting carried out.","2020-11-30","","Completed","2020-11-23","No","No","No","Internal"]
[null,null,null,null,14737,"23_11/11/2020 12:22:08 PM","2020-11-11","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ENGINE ROOM ACCESS  DOOR(FROM UPP DECK PASSAGE) PACKING CLEARIENCE IS EXCESSIVE.","Miscellaneous","General Appearance","Behaviour Based","10.44","Medium","","","DOOR FRAME NEED TO REPAIR AND PACKING NEEDS RENEWAL.","2020-11-15","","Completed","2020-11-12","No","No","No","Internal","complete as planned and close out"]
[null,null,null,null,16785,"23_05/01/2021 1:06:24 PM","2020-11-11","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Hydraulic boxes on deck need derusting and painting","Deck - Pipe / Fittings","General Appearance","External Factors","11.4","Very High","","","Derusting and painting carried out.","2020-12-31","","Completed","2020-12-22","No","No","No","Internal"]
[null,null,null,null,14738,"23_11/11/2020 12:26:47 PM","2020-11-11","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","VENTILLATION LOUVRES RUSTED IN EGCS SCRUBBER ROOM.","Miscellaneous","General Appearance","Behaviour Based","12.16","High","","","Derusting and painting carried out.","2021-01-31","","Completed","2020-12-15","No","No","No","Internal","complete as planned and close out"]
[null,null,null,null,16786,"23_05/01/2021 1:38:17 PM","2020-11-11","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Slop transfer line on the accommodation stbd side entrance, wasted, Chip and paint, renew as required.","Deck - Pipe / Fittings","General Appearance","External Factors","11.4","Very High","","","Derusting and painting carried out.","2020-11-30","","Completed","2020-11-23","No","No","No","Internal"]
[null,null,null,null,14739,"23_16/11/2020 1:33:06 AM","2020-11-11","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Mooring winches have rust marks. Need derusting and painting","Deck - Mooring Machinery","Mooring","External Factors","9.14","Medium","","","Derusting of winches completed","2021-03-31","","Completed","2021-03-15","No","No","No","Internal","complete as planned and close out"]
[null,null,null,null,14740,"23_16/11/2020 1:35:29 AM","2020-11-11","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","both windlass need derusting and painting","Deck - Mooring Machinery","Mooring","External Factors","9.2","Very High","","","Completed Derusting and painting.","2021-03-31","","Completed","2021-03-01","No","No","No","Internal","complete as planned and close out. \nwork in progress"]
[null,null,null,null,14741,"23_16/11/2020 1:38:42 AM","2020-11-11","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Both windlass Spurling pipe cover badly rusted. Both covers to be renewed.","Miscellaneous","General Appearance","External Factors","9.2","Very High","","","New cover fabricated.","2020-12-11","","Completed","2020-12-11","No","No","No","Internal"]
[null,null,null,null,14746,"23_11/11/2020 12:15:22 PM","2020-11-11","Defect","Ship Staff","Ship Staff Insp.","NO 2 D/G ALTERNATOR  DRIVE END BEARING TEMP SHOWING HIGH.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","ALL 3 DG ALTERNATOR BEARINGS(DRIVE END & NON DRIVE END)OIL RENEWED .GENERATOR TAKEN ON LOAD FOR 710 KW AND CHECKED TEMP ,FOUND SATISFACTORY AND IN LIMITS.","2020-12-31","","Completed","2020-11-15","No","No","No","Internal"]
[null,null,null,null,14742,"23_15/11/2020 3:34:02 PM","2020-11-14","Defect","Ship Staff","Ship Staff Insp.","STBD ECDIS  DISPLAY MONITOR NOT WORKING.","Navigation - ECDIS","Navigation","Equipment Related","","","","","OPENED UP THE DISPLAY AND FOUND THAT THE INSIDE PANEL BOARD BURNT,SAME NEW DISPLAY TO BE ORDERED AND TO RENEW.","2021-01-07","DHAW200248","Completed","2020-12-29","No","No","No","Internal","spare connected last call Singapore: complete and close out"]
[null,null,null,null,15417,"23_23/11/2020 3:37:36 AM","2020-11-16","Defect","Ship Staff","Ship Staff Insp.","Hydraulic leak observed from the Actuator of the valves BW-V823 / BW-V813 & BW-V831 - Open side in Pumproom.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.11","Medium","","","Actuator Seal of the valves BW-V823 / BW-V813 & BW-V831 - Open side in Pumproom replaced. tested no leak observed.","2020-11-22","","Completed","2020-11-18","No","No","No","Internal"]
[null,null,null,null,14744,"23_16/11/2020 1:13:06 AM","2020-11-16","Defect","Ship Staff","Ship Staff Insp.","Pumproom Davit wire found damage strands on top end","Miscellaneous","General Appearance","External Factors","5.2","Very High","","","Davit wire replaced with new wire","2021-01-09","DHAW200260","Completed","2020-12-30","No","No","No","Internal","wire supplied at Singapore; complete the job and close out"]
[null,null,null,null,14735,"23_11/11/2020 11:50:44 AM","2020-11-17","Defect","Ship Staff","Ship Staff Insp.","SEA WATER INLET & OUTLET VALVES DEFECTIVE FOR SWITCHBOARD ROOM/ECR AC  UINTS.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Inlet and outlet valves replaced with new ones.","2021-02-17","","Completed","2021-02-15","No","No","No","Internal","complete as planned and close out. \nspare valves onboard"]
[null,null,null,null,15412,"23_29/11/2020 9:04:25 PM","2020-11-25","Defect","Ship Staff","Ship Staff Insp.","ME LUBE OIL COOLER SEA WATER INLET PIPE T-JUNCTION GOT HOLE AND LEAKING","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","New Pipe renewedand fitted back.","2020-12-30","","Completed","2020-12-17","No","No","No","Internal","plan the job at Singapore along with other ME jobs"]
[null,null,null,null,15413,"23_29/11/2020 9:07:22 PM","2020-11-26","Defect","Ship Staff","Ship Staff Insp.","No 1 & no 2 boiler auto feed line valves to check & solve the problem with maintaining water level.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Boiler #1 auto feed valve removed from place and seat and stem renewed","2021-02-01","","Completed","2021-01-07","No","No","No","Internal","valves inspected and query for spare vv seals and poppets valve floated"]
[null,null,null,null,16544,"23_21/12/2020 10:03:40 PM","2020-12-01","Defect","Ship Staff","Ship Staff Insp.","During cargo operation and deballasting operation,taking pumproom rounds, leak was observed from the spool piece between WBP#1 and strainer at Fujairah SBM.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.21","High","","","Deballasting from the Line-1 was stopped and line drained. Later in the passage inspection of spool piece carried out and found due to corrosion in side the pipe hole was developed. Hole was build up by welding in E/R workshop and spool piece fitted back, tested no leaks observed.","2020-12-06","","Completed","2020-12-05","No","No","No","Internal"]
[null,null,null,null,16545,"23_21/12/2020 9:56:02 PM","2020-12-02","Observation","Ship Staff","Ship Staff Insp.","Inspection of FW / DW & A{T vent head carried out, Found cracks on the side plate of the vent head.","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","External Factors","11.7","High","","","Removed side plate of the vent head and maintenance carried out in E/R workshop, Derusting and painting done and fitted back.","2020-12-04","","Completed","2020-12-02","No","No","No","Internal"]
[null,null,null,null,16546,"23_21/12/2020 9:40:00 PM","2020-12-10","Observation","Ship Staff","Ship Staff Insp.","5C PV v/v one from pressure side and other from Vac. side found leaking","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.21","High","","","Both side of PV v/v replaced with the o'hauled PV v/v and fitted back, checked no leaks observed","2020-12-16","","Completed","2020-12-16","No","No","No","Internal"]
[null,null,null,null,16547,"23_21/12/2020 9:50:42 PM","2020-12-10","Observation","Ship Staff","Ship Staff Insp.","Foam monitor valve no.5 found leaking","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.35","Medium","","","Foam monitor vlave removed and inspected found wasted/corrosion  from inside, replaced with new vlave. tested no leaks observed.","2020-12-15","","Completed","2020-12-14","No","No","No","Internal"]
[null,null,null,null,16548,"23_21/12/2020 9:42:52 PM","2020-12-10","Defect","Ship Staff","Ship Staff Insp.","No. 1 Hydraulic power pack oil cooler outlet pipe foound leaking.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Pipe removed and fabricated new pipe, fitted back and tested, no leaks observed","2020-12-13","","Completed","2020-12-12","No","No","No","Internal"]
[null,null,null,null,16549,"23_21/12/2020 9:36:02 PM","2020-12-11","Defect","Ship Staff","Ship Staff Insp.","MGPS sea water line to High seachest found leaking","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Pipe removed from the place and fabricated new pipe and fitted back, no leaks observed","2020-12-15","","Completed","2020-12-14","No","No","No","Internal"]
[null,null,null,null,16550,"23_21/12/2020 9:29:30 PM","2020-12-13","Defect","Ship Staff","Ship Staff Insp.","M7 mooring winch pipe slight oil leaking from the return line connected after the winch motor.","Deck - Mooring Machinery","Mooring","Equipment Related","9.14","Medium","","","Return line pipe was removed, found pin hole and new pipe fabricated and fixed back tested no leaks observed. Later pipe was painted from outerside with 3 coats, primer and top coat green.","2020-12-16","","Completed","2020-12-16","No","No","No","Internal"]
[null,null,null,null,16541,"23_21/12/2020 10:35:04 PM","2020-12-16","Defect","Ship Staff","Ship Staff Insp.","Main engine starting air,cooling water,T/C#2 L.O. pressure gauges faulty","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Pressure gauges renewed","2021-02-16","","Completed","2020-12-23","No","No","No","Internal","raise RO and  replace TC #2 faulty with non essential machine for the mean while.\ninclude RO number in the DDRL"]
[null,null,null,null,16542,"23_21/12/2020 10:40:17 PM","2020-12-17","Defect","Ship Staff","Ship Staff Insp.","H.F.O. settling and service tank level gauges found faulty","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Requistion Number DHAW 210028 received at gola and gauges renewed.","2021-05-25","DHAW210028","Completed","2021-05-23","No","No","No","Internal","raise RO and include the same in DDRL as well.\nit will be processed once rcd in PAL."]
[null,null,null,null,16543,"23_22/12/2020 6:32:12 AM","2020-12-18","Defect","Ship Staff","Ship Staff Insp.","Scrubber cooling seawater pump outlet pipe holed and leaking","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.31","Very High","","","Pipe removed from place repaired by welding  and fitted back.Jig made for spare pipe and new pipe fabrication in progress.","2021-02-18","","Completed","2021-01-11","No","No","No","Internal","consider priority. seek shore assistance if required when ship calling convenient port"]
[null,null,null,null,16787,"23_05/01/2021 2:42:36 PM","2020-12-23","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Aircon external unit wire connection to bridge room on Stbdside is not water tight.","Accommodation,Elect. Mach. & Equip.","Structural Condn. / WT integrity ","Human Error","11.1","High","","","Putty inserted.","2020-12-31","","Completed","2020-12-31","No","No","No","Internal"]
[null,null,null,null,16704,"23_05/01/2021 10:29:58 AM","2020-12-24","Observation","Owner / Marine / Tech. Suptd.","Ship Staff Insp.","WBT 5P and 5S entrance is heavily corroded.","Hull & Tanks","Structural Condn. / WT integrity ","External Factors","11.6","Medium","","","Spot Derusting/Painting carried out","2021-02-28","","Completed","2021-02-19","No","No","No","Internal","carry out the job as per planned and complete by target date. works in progress"]
[null,null,null,null,16705,"23_05/01/2021 10:58:36 AM","2020-12-24","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","C deck stbd side exit door is corroded, damaged and wasted at the lower part.","Accommodation","General Appearance","External Factors","11.6","Medium","","","Maintenance/ painting carried out.","2021-03-31","","Completed","2021-02-22","No","No","No","Internal","Raise RO for the complete door, Spare to be arranged as per RO. it has lead time of about 2~3 M"]
[null,null,null,null,16707,"23_05/01/2021 11:01:34 AM","2020-12-24","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Monkey bridge Christmas tree and other antenna post is discolored with rust marks and spots","Miscellaneous","General Appearance","External Factors","11.8","Low","","","Derusting and painting carried out.","2021-01-31","","Completed","2021-01-31","No","No","No","Internal","carry out the job as per planned and complete by target date"]
[null,null,null,null,16708,"23_05/01/2021 11:40:30 AM","2020-12-24","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Port side accommodation ladder has a damaged plate below the steps at 2 places","Miscellaneous","Structural Condn. / WT integrity ","External Factors","5.47","Medium","","","Maintenance carried out, new plate inserted and painted.","2021-03-31","","Completed","2021-02-27","No","No","No","Internal","carry out the job as per planned and complete by target date."]
[null,null,null,null,16709,"23_05/01/2021 11:43:31 AM","2020-12-24","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Hospital weather door corroded","Accommodation","Structural Condn. / WT integrity ","External Factors","11.6","Medium","","","New door rcvd in singapore on 18 Aug 2021. Old door & frame removed and new one put in place. Door & frame painted with primer & TC","2021-05-08","DHAW210008","Completed","2021-08-27","No","No","No","Internal","spars in transit to Singapore; will be connected to ship at Singapore next call."]
[null,null,null,null,16710,"23_05/01/2021 11:47:42 AM","2020-12-24","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","One minor leak from stbd windlass winch control lever","Deck - Mooring Machinery","Mooring","External Factors","9.14","Medium","","","seal renewed , no leaks observed.","2021-04-15","DHAW 210045","Completed","2021-04-14","No","No","No","Internal","to be completed on receipt of spares on priority and close out"]
[null,null,null,null,16711,"23_05/01/2021 11:50:28 AM","2020-12-24","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Both anchor brakes tightening studs close to max limit","Deck - Machinery","Mooring","Equipment Related","9.14","Medium","","","Attempted to adjust the stud. But could not turn the adjusting screw as the same is in such as position that does not provide leverage. Also the adjusting screw is frozen","2021-03-24","","Completed","2021-11-21","No","No","No","Internal","minor adjustment done and rest planned for docking early 2022"]
[null,null,null,null,16712,"23_05/01/2021 2:48:58 PM","2020-12-24","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Aircon fresh air vest is heavily corroded, damage and dead flies are deposited","Accommodation","General Appearance","External Factors","11.8","Low","","","Derusting and painting carried out, air vest cleaned","2021-02-28","","Completed","2021-02-22","No","No","No","Internal","carry out the job as per planned and complete by target date"]
[null,null,null,null,16713,"23_05/01/2021 2:51:10 PM","2020-12-24","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Two bunker save all around accommodation - head area steel wasted","Deck - Pipe / Fittings","General Appearance","External Factors","6.9","Low","","","Derusting and painting carried out,wasted portion galvanised steel plate rivetted.","2021-01-31","","Completed","2021-02-18","No","No","No","Internal","replace the corroded plate with damaged edges"]
[null,null,null,null,16714,"23_05/01/2021 3:17:41 PM","2020-12-24","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","A/E fresh water cooler tray scupper choked and the minor drain lines choked with water","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.31","Very High","","","Pipe choke cleared,drain lines cleared ,salt deposits removed and pipes painted.","2021-02-24","","Completed","2021-02-06","No","No","No","Internal","carry out the job as per planned and complete by target date"]
[null,null,null,null,16715,"23_05/01/2021 3:19:57 PM","2020-12-24","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Inspect E.G.B. lower hopper for steel wastage-outside sign of exhaust leakage","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","New pipe section fabricated and fitted. Leak rectified","2021-03-15","","Completed","2021-02-15","No","No","No","Internal","anchorage job, plan before loading if time permits"]
[null,null,null,null,16716,"23_05/01/2021 3:21:48 PM","2020-12-24","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Protection for service air compressor to be fabricated and fitted for leakage from exhaust gas boiler.","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","New line fabricated in workshop  and fitted in place of leaking exhaust gas boiler line,hence no protection required for service air compressor ","2021-02-24","","Completed","2021-01-24","No","No","No","Internal"]
[null,null,null,null,16717,"23_05/01/2021 3:27:08 PM","2020-12-24","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Water leak below hypermist pump and solenoid block panel.","LSA / FFA","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Checked for leakage found leaking from citadel fresh water line, same rectified,found no further leak. ","2021-02-02","","Completed","2021-01-10","No","No","No","Internal","carry out the job as per planned and complete by target date"]
[null,null,null,null,16718,"23_05/01/2021 3:23:44 PM","2020-12-24","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","A/E#1 turbocharger cladding having sign of exhaust gas leakage.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Exhaust gas line cladding and lagging opened,nut and bolts tightened,auxiliary engine tried out,found no leakage.Lagging and cladding put back,found satisfactory.","2021-01-31","","Completed","2021-01-12","No","No","No","Internal","priority job- carry out the job as per planned and complete by target date"]
[null,null,null,null,16788,"23_05/01/2021 9:55:53 AM","2020-12-24","Observation","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","Outer packing channel plate of CO2 room weather tight door was wasted and corroded and piece of approximately 4 inches was worn out. Outer and inner channel plates of emergency generator room ventilator weather tight door\n\nwas corroded and wasted. A piece of inner channel of approximately 6 inches was worn out and hole of approximately 10 mm diameter noted on the outer channel.\n\n","Miscellaneous","General Appearance","External Factors","11.6","Medium","","","Maintenance on the CO2 room door carried out and door painted.","2020-12-31","","Completed","2020-12-29","No","No","No","External"]
[null,null,null,null,16789,"23_05/01/2021 9:59:48 AM","2020-12-24","Observation","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","Two of the closed chocks at the forecastle deck port quarter were moderately grooved by approximately 5 mm.  ","Deck - Mooring Machinery","Mooring","Equipment Related","9.18","Low","","","Grooving area build up with welding","2020-12-31","","Completed","2020-12-29","No","No","No","External"]
[null,null,null,null,16790,"23_05/01/2021 11:07:46 AM","2020-12-24","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Crew smoke room is totally dirty and celling and bulkheads are covered with dark layer of carbon","Accommodation","General Appearance","Human Error","11.13","Low","","","Cleaning of the crew smoke room carried out. ","2020-12-31","","Completed","2020-12-26","No","No","No","Internal"]
[null,null,null,null,16791,"23_05/01/2021 11:17:51 AM","2020-12-24","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Oxy-acetylene store door is heavily corroded","Miscellaneous","General Appearance","External Factors","5.26","Medium","","","Derusting and painting carried out.","2020-12-31","","Completed","2020-12-31","No","No","No","Internal"]
[null,null,null,null,16792,"23_05/01/2021 11:25:48 AM","2020-12-24","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Paint room is scattered, Need to be arranged","Miscellaneous","General Appearance","Human Error","5.46","Medium","","","Vessel received new paint during inspection, which were kept inside paint store, All newly paint drum arranged and stored in place.","2020-12-25","","Completed","2020-12-25","No","No","No","Internal"]
[null,null,null,null,16793,"23_05/01/2021 11:29:18 AM","2020-12-24","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Base points of the Fire extinguisher box beside oxy-acetylene bottle store is heavily corroded","LSA / FFA","Safety / LSA / FFA","External Factors","5.35","Medium","","","Derusting and painting carried out.","2020-12-31","","Completed","2020-12-31","No","No","No","Internal"]
[null,null,null,null,16794,"23_05/01/2021 11:31:17 AM","2020-12-24","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Portside life board embarkation platform grating is corroded","Hull & Tanks","General Appearance","External Factors","11.3","Medium","","","Derusting and painting carried out","2020-12-31","","Completed","2020-12-31","No","No","No","Internal"]
[null,null,null,null,16795,"23_05/01/2021 3:14:28 PM","2020-12-24","Other","Owner / Marine / Tech. Suptd.","Ship Staff Insp.","E.G.C.S. sick unit control air found to have water ingress","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Already fabricated air line with flanges  in workshop and auto drain filter  fitted near the entrance of E.G.C.S room.","2021-01-20","","Completed","2021-01-03","No","No","No","Internal"]
[null,null,null,null,16797,"23_05/01/2021 9:36:55 AM","2020-12-24","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Poop deck aft navigation light stand is corroded and rusty","Miscellaneous","General Appearance","External Factors","11.8","Low","","","Derusting and painting carried out.","2021-01-31","","Completed","2020-12-30","No","No","No","Internal"]
[null,null,null,null,15414,"23_29/11/2020 9:12:24 PM","2020-12-27","Defect","Ship Staff","Ship Staff Insp.","Main engine air cooler no 1 sea water outlet pipe having doubler, same pipe to be renewed.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.31","Very High","","","pipe to be renewed.","2021-03-15","","Completed","2021-06-30","No","No","No","Internal","one pipe renewed at Singapore last call, plan to renew before the load port mid Jan 21\nrubber coated pipe supplied in Singapore"]
[null,null,null,null,16796,"23_05/01/2021 12:14:04 PM","2020-12-29","Defect","Ship Staff","Ship Staff Insp.","FW pipe leaking near 2C area on main deck.","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","External Factors","11.4","Very High","","","Wasted pipe fabricated and fitted back. Tested, no leak observed.","2020-12-31","","Completed","2020-12-31","No","No","No","Internal"]
[null,null,null,null,18036,"23_01/03/2021 10:48:17 AM","2021-01-01","Observation","Ship Staff","Ship Staff Insp.","Descaling and painting need to be done on the poop deck","Deck - Pipe / Fittings,Hull & Tanks","General Appearance","External Factors","11.3","Medium","","","Descaling and painting on the poop deck completed.","2021-02-28","","Completed","2021-02-21","No","No","No","Internal"]
[null,null,null,null,18037,"23_01/03/2021 10:51:33 AM","2021-01-01","Observation","Ship Staff","Ship Staff Insp.","Rust on the port manifold walkway area need to be derusted and painted.","Deck - Pipe / Fittings,Hull & Tanks","General Appearance","External Factors","11.3","Medium","","","Descaling and painting on the port manifold walkway area completed","2021-02-28","","Completed","2021-01-25","No","No","No","Internal"]
[null,null,null,null,18038,"23_01/03/2021 10:53:55 AM","2021-01-01","Observation","Ship Staff","Ship Staff Insp.","Rust on the 2P deck area, need to Descale and paint","Deck - Pipe / Fittings,Hull & Tanks","General Appearance","External Factors","11.3","Medium","","","Descaling and painting on the 2P area completed","2021-02-28","","Completed","2021-02-28","No","No","No","Internal"]
[null,null,null,null,17427,"23_18/01/2021 12:55:45 AM","2021-01-05","Defect","Ship Staff","Ship Staff Insp.","Slop-P IG valve not holding.","Deck - Pipe / Fittings,Inert Gas","Cargo / Ballast Systems","Equipment Related","8.31","High","","","Valve replaced with new valve. found holding.","2021-01-22","","Completed","2021-01-12","No","No","No","Internal"]
[null,null,null,null,17428,"23_18/01/2021 12:57:42 AM","2021-01-05","Observation","Ship Staff","Ship Staff Insp.","1C PV valve found leaking","Deck - Pipe / Fittings,Inert Gas","Cargo / Ballast Systems","Equipment Related","8.21","High","","","Replaced with overhauled PV valve, found holding and no leaks","2021-01-22","","Completed","2021-01-10","No","No","No","Internal"]
[null,null,null,null,17432,"23_18/01/2021 1:00:40 AM","2021-01-05","Defect","Ship Staff","Ship Staff Insp.","Hydraulic leak from Actuator on BW-V831 (Openside) / 825 (Open/close side) & COV 513 v/v (Close side)  ","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.11","Medium","","","Seal repalced and operated vlaves, noleaks observed.","2021-01-22","","Completed","2021-01-16","No","No","No","Internal"]
[null,null,null,null,17429,"23_12/01/2021 9:59:17 PM","2021-01-06","Observation","Ship Staff","Ship Staff Insp.","IG line dressor coupling fwd and aft of Mastriser & aft of PV breaker need to be inspected and replace.","Deck - Pipe / Fittings,Inert Gas","Cargo / Ballast Systems","Equipment Related","8.3","Very High","","","Inspection of IG line dressor coupling carried out, replaced with new seal ring.","2021-01-31","","Completed","2021-01-13","No","No","No","Internal"]
[null,null,null,null,17430,"23_12/01/2021 8:42:45 PM","2021-01-07","Observation","Ship Staff","Ship Staff Insp.","Foam Isolation v/v near F/monitor # 6, found hard to operate.","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.38","High","","","Maintennace on the Isolation valve carried out, found moving freely.","2021-01-15","","Completed","2021-01-11","No","No","No","Internal"]
[null,null,null,null,17431,"23_16/01/2021 4:40:56 PM","2021-01-11","Defect","Ship Staff","Ship Staff Insp.","Fuel oil auto backwash filter found leaking oil from the air line,during the backflushing process.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Bottom sludge discharge valve and solenoid valves  o'hauled,air solenoid valve for pneumatic swivel drive o'hauled,filter elements replaced with cleaned ones,tried out,found no leakage.","2021-01-18","","Completed","2021-01-15","No","No","No","Internal"]
[null,null,null,null,17718,"23_05/02/2021 3:47:59 AM","2021-01-19","Defect","Ship Staff","Ship Staff Insp.","EGB hopper drain line above control air compressor  found leaking ","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.31","Very High","","","Existing Pipe jig made in workshop,new pipe  fabricated fitted and tried out.","2021-02-11","","Completed","2021-01-24","No","No","No","Internal"]
[null,null,null,null,17719,"23_06/02/2021 1:45:42 AM","2021-01-22","Breakdown","Ship Staff","Ship Staff Insp.","The engine room crane hoisting motor was tripping on overload when the hoisting/lowering switch is being pressed.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","After troubleshooting,found hoisting motor shaft was bent and had a wobble of 0.4mm .The engine room crane motor shaft was machined on lathe and the diameter of the shaft was reduced by 0.2mm,the shaft was checked for trueness again the wobble was reduced to 0.04mm.The long connecting shaft was also checked for trueness found in good condition.Crane motor and shaft fitted back in place and tried out,found satisfactory.","2021-02-10","","Completed","2021-02-04","No","No","No","Internal"]
[null,null,null,null,17720,"23_01/02/2021 1:30:27 AM","2021-01-25","Observation","Ship Staff","Ship Staff Insp.","Foam isolation valve no. 1 found hard to operate","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.38","High","","","Maintenance on Foam Isolation valve carried out, moving freely","2021-01-31","","Completed","2021-01-30","No","No","No","Internal"]
[null,null,null,null,17721,"23_05/02/2021 3:54:29 AM","2021-01-25","Defect","Ship Staff","Ship Staff Insp.","Main engine lube oil cooler sea water inlet distance piece chemical cleaning pipe found leaking ","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.31","Very High","","","The distance piece was renewed with a spare one which was already fabricated and kept as spare ","2021-01-28","","Completed","2021-01-27","No","No","No","Internal"]
[null,null,null,null,17849,"23_18/02/2021 6:31:32 PM","2021-02-01","Defect","Ship Staff","Ship Staff Insp.","Fresh water generator and main engine jacket water coolers common drain line found choked and leaking ","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.31","Very High","","","Drain pipe removed from place taken to workshop,new pipe fabricated and fitted back in place ","2021-02-28","","Completed","2021-02-10","No","No","No","Internal"]
[null,null,null,null,17850,"23_10/02/2021 3:16:54 PM","2021-02-02","Defect","Ship Staff","Ship Staff Insp.","Pin hole observed on IG Line dressor coupling ring. ","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.3","Very High","","","Inspection and maintenance work carried out &  seal ring replaced.","2021-02-10","","Completed","2021-02-09","No","No","No","Internal"]
[null,null,null,null,18039,"23_01/03/2021 2:27:04 PM","2021-02-05","Defect","Ship Staff","Ship Staff Insp.","MW-7 winch control lever found leaking ","Deck - Machinery","Mooring","Equipment Related","9.14","Medium","","","Lever oil  seal and o-rings renewed ","2021-02-28","","Completed","2021-02-23","No","No","No","Internal"]
[null,null,null,null,17851,"23_18/02/2021 6:42:11 PM","2021-02-07","Other","Ship Staff","Ship Staff Insp.","E.C.R. Air conditioning system found tripping on high pressure.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.31","Very High","","","Found outlet pipe choked.Section of pipe removed from place,choke cleared ,fitted back and tried out.","2021-02-13","","Completed","2021-02-11","No","No","No","Internal"]
[null,null,null,null,17847,"23_21/02/2021 9:17:44 PM","2021-02-08","Defect","Ship Staff","Ship Staff Insp.","No#1 steering gear chain coupling cover found cracked during routine inspection.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Cover repaired and fitted back.","2021-04-12","DHAW210059","Completed","2021-04-06","No","No","No","Internal","spares onboard, kindly carry out the replacement on priority."]
[null,null,null,null,17848,"23_21/02/2021 9:14:07 PM","2021-02-10","Defect","Ship Staff","Ship Staff Insp.","No#4 deck machinery hydraulic pump discharge pressure gauge faulty.","Deck - Mooring Machinery","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Pressure gauge  renewed ","2021-03-31","DHAW210044","Completed","2021-03-15","No","No","No","Internal","spare gauge to be arranged ; two  pr gauge also available under winch tools."]
[null,null,null,null,17854,"23_18/02/2021 6:37:33 PM","2021-02-11","Defect","Ship Staff","Ship Staff Insp.","Switch board cooler inlet sea water line found leaking ","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.31","Very High","","","Pipe dimensions taken,new pipe fabricated, fitted in place and tried out","2022-02-28","","Completed","2021-02-15","No","No","No","Internal"]
[null,null,null,null,17852,"23_18/02/2021 6:44:53 PM","2021-02-12","Defect","Ship Staff","Ship Staff Insp.","E.C.R. and switch board rooms drain line in bottom platform found choked and leaking ","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.31","Very High","","","Pipe taken to workshop,new pipe fabricated and fitted.","2021-03-07","","Completed","2021-02-20","No","No","No","Internal"]
[null,null,null,null,17853,"23_18/02/2021 6:49:39 PM","2021-02-14","Other","Ship Staff","Ship Staff Insp.","Fresh water generator production found dropping to 18 MT/day due to scaling of the evaporator ","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Fresh water generator stopped,isolated,cleaned with descaling liquid by circulation.Fresh water generator tried out,found production to be 24 mt/day","2021-02-20","","Completed","2021-02-15","No","No","No","Internal"]
[null,null,null,null,18040,"23_22/02/2021 5:42:09 PM","2021-02-16","Defect","Ship Staff","Ship Staff Insp.","Pin hole observed from Main IG line near 5C.","Deck - Pipe / Fittings,Inert Gas","Cargo / Ballast Systems","Equipment Related","8.3","Very High","","","Coldwork carried out.","2021-02-28","","Completed","2021-02-16","No","No","No","Internal"]
[null,null,null,null,18041,"23_22/02/2021 5:48:30 PM","2021-02-16","Defect","Ship Staff","Ship Staff Insp.","Ballast level gauge showing erratic reading.","Deck - Pipe / Fittings","Cargo / Ballast Systems","External Factors","8.13","Medium","","","Ballast level gauge line on main deck checked and found pipe cracked near under the clamp fitting where the air in th epipe was leaking. Clamp was removed to inspect the condition and found line cracked at 3 places. ermato coupling fixed and  leak was arrested.","2021-02-28","","Completed","2021-02-24","No","No","No","Internal"]
[null,null,null,null,18042,"23_28/02/2021 19:38:39","2021-02-16","Observation","Ship Staff","Ship Staff Insp.","COW line dressor coupling seal rings to be replaced.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.34","High","","","Replacement of seal ring of COW dressor coupling  x 3 nos. carried out.","2021-02-28","","Completed","2021-02-21","No","No","No","Internal"]
[null,null,null,null,18043,"23_28/02/2021 19:26:42","2021-02-25","Defect","Ship Staff","Ship Staff Insp.","BW-V223 Stripper v/v of 3P WBT found leaking from actuator during inspection.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.11","Medium","","","Seal replaced and tested no leaks observed","2021-02-26","","Completed","2021-02-25","No","No","No","Internal"]
[null,null,null,null,18278,"23_15/03/2021 8:36:06 AM","2021-03-05","Observation","Ship Staff","Ship Staff Insp.","Port Accommodation ladder swing in/out control pneumatic valve faulty","Deck - Machinery","General Appearance","Equipment Related","5.47","Medium","","","Pipes renewed and tried out, working satisfactorily.","2021-11-30","","Completed","2021-10-20","No","No","No","Internal","Raise RO on priority"]
[null,null,null,null,18279,"23_14/03/2021 6:32:58 PM","2021-03-07","Defect","Ship Staff","Ship Staff Insp.","Galley ac cooling water inlet pipe found leaking in AC blower room","Accommodation","Eng. / Strg. Comp.","Equipment Related","10.31","Very High","","","Spare pipe fabricated and kept stdby,to be changed at next available opportunity.","2021-04-15","","Completed","2021-04-10","No","No","No","Internal","complete as planned and close out"]
[null,null,null,null,18280,"23_14/03/2021 6:36:01 PM","2021-03-08","Other","Ship Staff","Ship Staff Insp.","No#2 boiler water circulating pump differential pressure found to be 0.35 bar","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Circulating pump removed from place , impeller cleaned of rust and debris .Pump fitted and tried out.","2021-03-10","","Completed","2021-03-09","No","No","No","Internal"]
[null,null,null,null,18281,"23_14/03/2021 6:40:48 PM","2021-03-09","Defect","Ship Staff","Ship Staff Insp.","NO:1 And No:2 boiler uptake valves for inertgas plant found seized","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Inspection covers for both valves removed,valve flaps cleaned,eased up,actuator fitted and tried out.","2021-03-12","","Completed","2021-03-11","No","No","No","Internal"]
[null,null,null,null,18277,"23_14/03/2021 6:47:14 PM","2021-03-10","Defect","Ship Staff","Ship Staff Insp.","Port boiler solenoid valve for sealing air of uptake valve  found faulty","Inert Gas","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Solenoid valve replaced with spare.","2021-06-02","DHAW210099","Completed","2021-08-23","No","No","No","Internal","RO is processed, awaiting readiness"]
[null,null,null,null,18282,"23_14/03/2021 6:49:52 PM","2021-03-10","Other","Ship Staff","Ship Staff Insp.","Sludge pump found to be taking more time to top up incinerator waste oil tanks ","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Sludge pump o'hauled,stator renewed ","2021-03-15","","Completed","2021-03-12","No","No","No","Internal"]
[null,null,null,null,18283,"23_15/03/2021 8:28:46 AM","2021-03-12","Observation","Ship Staff","Ship Staff Insp.","Fire and Foam dressor coupling found leaking.","Deck - Pipe / Fittings,LSA / FFA","Safety / LSA / FFA","Equipment Related","5.35","Medium","","","Seal ring of the dressor coupling replaced and tested, found no leaks","2021-03-14","","Completed","2021-03-13","No","No","No","Internal"]
[null,null,null,null,18284,"23_15/03/2021 8:30:51 AM","2021-03-12","Observation","Ship Staff","Ship Staff Insp.","One foam and 2 Fire hydrant leaking.","Deck - Pipe / Fittings,LSA / FFA","Safety / LSA / FFA","External Factors","5.35","Medium","","","All leaking fire/foam hydrant repalced with O/H /New and tested, found no leaks.","2021-03-14","","Completed","2021-03-13","No","No","No","Internal"]
[null,null,null,null,18458,"23_04/04/2021 7:04:09 PM","2021-03-30","Breakdown","Ship Staff","Ship Staff Insp.","EGCS CEMS unit display failure, SICK unit fuse found blown","E/R - Main Engine","MARPOL Related","Equipment Related","10.32","Very High","","","CEMS unit- PCB replaced and problem solved.","2021-09-30","","Completed","2021-09-24","No","No","No","Internal","spares and serv tech to arrange once confirmed from makers HHI\nfollow up serv at Singapore on 20th.\nneed for additional spares, to attend ship again at Singapore around 26 Sept"]
[null,null,null,null,22016,"23_21/10/2021 2:14:00 PM","2021-03-31","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Marking of various Valves in Pump room missing and few are faded. New stencilling/ Marking of Valve number to be done. ","Deck - Pipe / Fittings","Cargo / Ballast Systems","Human Error","8.18","High","","","Valve  Markings in Pump room carried out for three Valves and four faded Valve nos. ","2021-04-14","","Completed","2021-04-04","No","No","No","Internal"]
[null,null,null,null,22017,"23_21/10/2021 2:17:25 PM","2021-03-31","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Fire Hydrant on Poop deck found having dripping leak.","LSA / FFA","Emgcy. Systems","Equipment Related","5.35","Medium","","","Fire hydrant overhauled and sealing face lapped. Tested and found satisfactory.","2021-04-14","","Completed","2021-04-05","No","No","No","Internal"]
[null,null,null,null,22018,"23_22-Oct-21 13:23:01","2021-03-31","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Stbd. Lifeboat Bilge pump suction hose to renew.","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.27","Medium","","","Stbd. L/B bilge pump suction hose renewed.","2021-04-03","","Completed","2021-04-01","No","No","No","Internal"]
[null,null,null,null,22019,"23_22-Oct-21 13:27:42","2021-03-31","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Air leak near port gangway control box to be rectified.","Deck - Machinery","Structural Condn. / WT integrity ","Equipment Related","5.47","Medium","","","Section of holed line replaced with newly fabricated line","2021-04-14","","Completed","2021-04-05","No","No","No","Internal"]
[null,null,null,null,22020,"23_22-Oct-21 13:32:55","2021-03-31","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","A/E used cy.head to be overhauled and keep ready to use","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Two no’s of cy.head overhauled and kept ready to use.","2021-04-07","","Completed","2021-04-04","No","No","No","Internal"]
[null,null,null,null,22021,"23_22-Oct-21 13:37:18","2021-03-31","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Steam leakage noticed from NO.1(S)HFO Bunker tk steam inlet valve flange.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","steam leakage rectified by renewing gasket.","2021-04-07","","Completed","2021-04-03","No","No","No","Internal"]
[null,null,null,null,22022,"23_22-Oct-21 13:43:05","2021-03-31","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Control air leakage from No.1 IG Blower discharge valve actuator.","Inert Gas","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Air leak from No.1  IG Blower discharge valve rectified.","2021-04-05","","Completed","2021-04-03","No","No","No","Internal"]
[null,null,null,null,22023,"23_22-Oct-21 13:46:49","2021-03-31","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","220V Low insulation activated,identify and rectify the fault.","Elect. Mach. & Equip.","Structural Condn. / WT integrity ","Equipment Related","10.24","Low","","","220v low insulation from upper dk(p) light,same rectified.","2021-04-05","","Completed","2021-04-02","No","No","No","Internal"]
[null,null,null,null,22024,"23_22-Oct-21 13:52:25","2021-03-31","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","No.1 Economiser feed water pump gland leaking.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Gland packing renewed,leakage stopped.","2021-04-05","","Completed","2021-04-02","No","No","No","Internal"]
[null,null,null,null,22025,"23_21/10/2021 7:27:53 PM","2021-03-31","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Housekeeping / through cleaning of Mid-ship locker and Changing lockers to be carried out. ","Accommodation","General Appearance","Behaviour Based,Human Error","10.29","Medium","","","Thorough cleaning and housekeeping carried out in Mid-Ship store and Changing locker.","2021-04-14","","Completed","2021-04-08","No","No","No","Internal"]
[null,null,null,null,20109,"23_17/07/2021 10:04:20 AM","2021-03-31","Observation","Owner / Marine / Tech. Suptd.","Cargo Audit","No master key for IG branch valves- Same observation in SIRE Mar-2021","Deck - Pipe / Fittings","Cargo / Ballast Systems","Inappropriate Procedure","8.2","Medium","","","Spare received and item closed out","2021-08-30","DHAW210213","Completed","2021-08-18","No","No","No","Internal"]
[null,null,null,null,19387,"23_02/05/2021 7:25:34 PM","2021-04-01","Observation","Ship Staff","Ship Staff Insp.","3S WBT gauge showing wrong reading in CCR","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","Leaking air in pneumatic line from foam room to sensor repaired","2021-07-31","","Completed","2021-05-14","No","No","No","Internal"]
[null,null,null,null,19388,"23_02/05/2021 7:23:46 PM","2021-04-01","Observation","Ship Staff","Ship Staff Insp.","4P WBT gauge is showing wrong reading in CCR","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","Leaking air from pneumatic line to the sensor repaired","2021-07-31","","Completed","2021-05-13","No","No","No","Internal","find and isolate the air leaks .\ncheck the air purge pipe in the WBT as well"]
[null,null,null,null,19389,"23_02/05/2021 9:18:54 PM","2021-04-02","Defect","Ship Staff","Ship Staff Insp.","Both f.w tanks level gauges not operational , no other means of gauging tank levels.","Deck - Pipe / Fittings","Eng. / Strg. Comp.","Equipment Related","","","","","DHAW 210026  Recived at gola , gauge renewed.","2021-05-30","","Completed","2021-05-26","No","No","No","Internal","spares confirmed and will be ready for connection soon"]
[null,null,null,null,19390,"23_02/05/2021 9:37:20 PM","2021-04-02","Defect","Ship Staff","Ship Staff Insp.","M/E FO SUPPLY PUMP DUPLEX FILTER CHANGE OVER HANDLE IS STUCK , REQUIRES M/E STOPPAGE AND DG TO BE CHANGED OVER TO LSMGO FOR CLEANING.","Deck - Pipe / Fittings","Eng. / Strg. Comp.","Equipment Related","","","","","During Vessel drifting,A/E f.o.sys c/o to LSMGO,then filter cleaned. C/O handle eased up.","2021-09-30","","Completed","2021-11-11","No","No","No","Internal","please make sure that the filter change over cock is jacked up before change over. revert is separate mail with drawing details."]
[null,null,null,null,19391,"23_02/05/2021 11:14:29 PM","2021-04-02","Defect","Ship Staff","Ship Staff Insp.","M/E F.O AUTOBACKWASH FILTER NOT BACK FLUSHING, DRAIN PISTON IS STUCK IN OPEN POSITION, 9 M3 OF OIL FILLING UP IN OVERFLOW TANK DAILY.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","DRAIN PISTON  OVERHAULED AND FREEd UP , back flushing operation confirmed.","2021-05-10","","Completed","2021-05-06","No","No","No","Internal","complete on priority and close out"]
[null,null,null,null,19392,"23_02/05/2021 11:18:16 PM","2021-04-02","Defect","Ship Staff","Ship Staff Insp.","BOTH INCINERATOR WASTE OIL TANKS LEVEL GAUGE MECHANISM MISSING FROM PLACE, UNABLE TO FIND OUT LEVEL IN TANKS.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","DHAW210136 RAISED FOR LEVEL GAUGES.","2021-05-30","","Completed","2021-08-30","No","No","No","Internal","No quotes available as no drawings and details available.\nvessel to continue with manual sounding"]
[null,null,null,null,19393,"23_02/05/2021 9:25:04 PM","2021-04-03","Defect","Ship Staff","Ship Staff Insp.","BOTTOM PLATFORM PLATES SECURING SCREWS MISSING","Miscellaneous","Eng. / Strg. Comp.","External Factors","","","","","PLATES TO BE SCRWED  AND MAKE SECURE.","2021-05-10","","Completed","2021-05-10","No","No","No","Internal","complete as planned and close out"]
[null,null,null,null,19394,"23_02/05/2021 9:28:25 PM","2021-04-03","Defect","Ship Staff","Ship Staff Insp.","SEWAGE CHANGE OVER VALVE IS STUCK","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","3-WAY VALVE EASED UP.","2021-08-27","","Completed","2021-11-17","No","No","No","Internal","complete as planned and close out"]
[null,null,null,null,19395,"23_02/05/2021 9:40:22 PM","2021-04-03","Defect","Ship Staff","Ship Staff Insp.","L.O PURIFIER #2 IS NOT OPERATIONAL","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","purifier assembly belt renewed , all components checked and operated found satisfactory","2021-05-30","","Completed","2021-05-20","No","No","No","Internal","revert in separate mail with details and current status"]
[null,null,null,null,19396,"23_02/05/2021 9:45:20 PM","2021-04-03","Defect","Ship Staff","Ship Staff Insp.","Fire and bilge pump not in use due to suction strainer casing corroded. Suction  or discharge valve may not be holding due to which unable to attend to strainer repairs.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Pump tried out in presence of class surveyor during class annuals.","2021-09-10","DHAW210199 raised for the valves","Completed","2021-08-21","Yes","No","No","Internal","spare casing supplied to ship and later reported no issues with the casing - case closed"]
[null,null,null,null,19397,"23_02/05/2021 9:32:05 PM","2021-04-04","Defect","Ship Staff","Ship Staff Insp.","BOTH BOILERS UNABLE TO MAINTAIN WATER LEVEL, CONTROLLER VALVES LEAKING INSPITE OF LAPPING .","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.31","Very High","","","Boiler #1 auto feed valve seat and stem renewed with new spare, valve performance noted good during cargo discharging operation. For No.2 Boiler,valve height adjusted at fully shut position,DP transmitter lines blown through,condensate pot filled with water and calibrated,found working satisfactorily.","2021-05-30","","Completed","2021-10-18","No","No","No","Internal","spares processed; lead time about 3 months, expected readiness June 21"]
[null,null,null,null,20107,"23_17/07/2021 9:47:06 AM","2021-04-05","Observation","Ship Staff","Ship Staff Insp.","Soft patch on IG line near 5C COT. Temporary repair carried out.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","","","","","Leaking section of the pipe repaired by hot work. Shall make entry in ref man to renew the section in next DD","2022-07-31","","Completed","2021-08-13","No","No","No","Internal"]
[null,null,null,null,20108,"23_17/07/2021 9:48:46 AM","2021-04-05","Observation","Ship Staff","Ship Staff Insp.","Soft patch on VECS line near port & stbd side cargo manifold area","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","","","","","Renewed the aft VECS line port & stbd side. Fwd side VECS line repaired at singapore by off landing the same to recreate marine. Pipe fitted back in place","2021-07-31","","Completed","2021-08-20","No","No","No","Internal"]
[null,null,null,null,20110,"23_17/07/2021 10:00:38 AM","2021-04-05","Breakdown,Observation","Ship Staff","Ship Staff Insp.","Stbd side hose handling crane runner limit faulty.","Deck - Machinery","Cargo / Ballast Systems","Equipment Related","8.5","Very High","","","Limit switch made operational. Hydraulic motor to be replaced at D/D.","2021-11-30","","Completed","2021-11-24","No","No","No","Internal","spares dispatched for connection at Fujairah -03 sept.\njob to be completed on priority"]
[null,null,null,null,19398,"23_02/05/2021 7:28:15 PM","2021-04-06","Observation","Ship Staff","Ship Staff Insp.","SLOP P IG press sensor faulty","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.19","High","","","Faulty sensor replaced with new sensor","2021-07-28","DHAW210137","Completed","2021-08-24","No","No","No","Internal","sensor processed for supply from Musasino."]
[null,null,null,null,19399,"23_02/05/2021 7:31:54 PM","2021-04-06","Observation","Ship Staff","Ship Staff Insp.","1C COT overfill alarm faulty","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.14","Very High","","","Require spare relay card to rectify the issue. Old resistance tape changed. Issue with the relay card","2021-07-30","DHAW210131","Completed","2021-08-20","No","No","No","Internal","spares processed from makers JOWA. procure trying to connect in US sub to lead time."]
[null,null,null,null,20211,"23_26/07/2021 8:32:53 AM","2021-04-06","Defect","Ship Staff","Ship Staff Insp.","Steering gear supply air trunking corroded / damaged.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","trunking section needs renewal. Defect transferred in REFMAN for DD.","2022-08-31","","Completed","2021-10-30","Yes","No","No","Internal"]
[null,null,null,null,20212,"23_01/08/2021 11:06:53 AM","2021-04-07","Defect","Ship Staff","Ship Staff Insp.","EGCS sea chest anodes not in place","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Anodes renewed and system put in service.","2021-09-25","DHAW210005","Completed","2021-09-04","No","No","No","Internal"]
[null,null,null,null,20111,"23_16/07/2021 4:27:15 PM","2021-04-08","Defect","Ship Staff","Ship Staff Insp.","#2 boiler uptake valve jammed / not moving manually or automatically","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Uptake valve overhauled by shore workshop, valve fitted in place and tried out. Comfirm smooth closing & opening operation","2021-09-30","","Completed","2021-08-20","No","No","No","Internal","Shore team to be arranged for overhauling at Singapore- aug 21"]
[null,null,null,null,20112,"23_16/07/2021 5:27:29 PM","2021-04-08","Defect","Ship Staff","Ship Staff Insp.","ME FO flowmeter defective.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Awaiting for spare DHAW210178.Also,flowmeter inlet v/v not holding,so job deferred to D/D.","2021-09-06","DHAW210178","Completed","2021-11-28","Yes","No","No","Internal"]
[null,null,null,null,19400,"23_02/05/2021 7:34:00 PM","2021-04-08","Observation","Ship Staff","Ship Staff Insp.","GPS position input into MF/HF not occuring automatically","Navigation - GMDSS & Communication","Communication","Equipment Related","","","","","Complete unit assembly for MF/HF- JSB-196GM Radiotelephony changed at Singapore. Automatic position issue resolved","2021-07-31","","Completed","2021-08-18","No","No","No","Internal","serv to be arrangement in progress at GOLA"]
[null,null,null,null,19401,"23_02/05/2021 7:36:42 PM","2021-04-08","Observation","Ship Staff","Ship Staff Insp.","CO2 room mushroom vents holed","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","Equipment Related","","","","","Removed to ER & repaired","2021-05-14","","Completed","2021-05-12","No","No","No","Internal","job completed, please close out"]
[null,null,null,null,20113,"23_17/07/2021 10:08:45 AM","2021-04-15","Defect,Observation","Ship Staff","Ship Staff Insp.","No 3 COP suction & discharge pressure gauges in PR are defective","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.13","Medium","","","New pressure gauge fitted and issue resolved","2021-08-30","DHAW210135","Completed","2021-08-19","No","No","No","Internal","Spares confirmed for supply at Singapore - 12 Aug"]
[null,null,null,null,19402,"23_02/05/2021 7:39:12 PM","2021-04-25","Observation","Ship Staff","Ship Staff Insp.","Emg generator weather tight door, channel lip fully wasted","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","Equipment Related","","","","","Wasted areas repaired","2021-05-14","","Completed","2021-05-12","No","No","No","Internal","close out as planned"]
[null,null,null,null,19918,"23_21/05/2021 5:45:52 AM","2021-05-15","Observation","Ship Staff","Ship Staff Insp.","Oil leak in VRCS ","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","12.2","High","","","Leaking actuators in pump room, deck cross over, ballast tanks opened. Leaking oil seal renewed. ","2021-08-30","","Completed","2021-08-14","No","No","No","Internal"]
[null,null,null,null,19919,"23_17/05/2021 8:53:52 PM","2021-05-17","Defect","Ship Staff","Ship Staff Insp.","2C COT overfill alarm faulty","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.14","Very High","","","faulty relay unit need renewal","2021-07-31","210131","Completed","2021-08-20","No","No","No","Internal","mention the RO , spares ready for connection."]
[null,null,null,null,19921,"23_19/05/2021 9:23:14 PM","2021-05-17","Observation","Ship Staff","Ship Staff Insp.","VRCS- Audio visual alarm for low pressure not working ","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","Find the fault & rectify the issue","2021-07-31","","Completed","2021-05-22","No","No","No","Internal"]
[null,null,null,null,20114,"23_16/07/2021 5:34:05 PM","2021-05-19","Defect","Ship Staff","Ship Staff Insp.","Valves for supply and circulating pumps in the ME and DG FO system not holding.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Defective valves to be renewed at  D/D. DHAW210199.","2021-09-14","DHAW210199","Completed","2021-11-27","Yes","No","No","Internal","spares onboard; complete the job at suitable opportunity"]
[null,null,null,null,20115,"23_17/07/2021 9:55:55 AM","2021-06-01","Observation","Ship Staff","Ship Staff Insp.","ODME calibration failure- Require spare halogen lamp","Cargo Mach.","MARPOL Related","Equipment Related","6.13","Low","","","Service tech attended the vessel who replaced the spares for ODME and carried out calibration and servicing of ODME on 18 Aug 2021","2021-08-30","DHAW210147","Completed","2021-08-18","No","No","No","Internal","annual ser also confirmed for Singapore from makers."]
[null,null,null,null,20122,"23_17/07/2021 9:57:43 AM","2021-06-01","Breakdown,Observation","Ship Staff","Ship Staff Insp.","ODME sampling p/p leaking due to worn out mechanical seal","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","Service tech attended the vessel who replaced the spares for ODME and carried out calibration and servicing of ODME on 18 Aug 2021","2021-08-30","DHAW210147","Completed","2021-08-18","No","No","No","Internal","spare seal confirmed for supply and at forwarders"]
[null,null,null,null,20116,"23_16/07/2021 4:16:47 PM","2021-06-02","Defect","Ship Staff","Ship Staff Insp.","M/E fuel oil autobackwash filter fuel oil passing through air cylinder and leaking out.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Bottom housing and ram renewed, filter boxed back and put in service.. No leak noted from the filter anymore","2021-09-30","DHAW210167","Completed","2021-09-04","No","No","No","Internal","spares processed for supply, followup with procure for supply at Singapore"]
[null,null,null,null,20117,"23_17/07/2021 10:11:09 AM","2021-06-02","Observation","Ship Staff","Ship Staff Insp.","Stbd side draft gauge slow in response","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","Sensor checked. Read out accurate. No leak of air. Read out during cargo discharging operations were satisafactory.","2021-08-30","","Completed","2021-07-26","No","No","No","Internal","write back with complete details if shore assistance required."]
[null,null,null,null,20520,"23_14/08/2021 9:54:00 AM","2021-06-04","Defect","Ship Staff","Ship Staff Insp.","ME FO AUTO filter FO is leaking past the bottom ram and entering the 5/2 valve air chamber. FO leaks during back flushing","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.36","Very High","","","Bottom drain RAM and valve housing to be renewed","2021-09-30","DHAW210167","Completed","2021-09-01","No","No","No","Internal"]
[null,null,null,null,20118,"23_17/07/2021 10:13:40 AM","2021-06-10","Observation","Ship Staff","Ship Staff Insp.","Float inside port & stbd side vent for APT amiss","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","Equipment Related","11.7","High","","","New float placed inside the vent head and item closed out","2021-08-30","DHAW210148","Completed","2021-08-22","No","No","No","Internal","it is a serious concern and close out on high priority."]
[null,null,null,null,20127,"23_16/07/2021 5:44:43 PM","2021-06-15","Defect","Ship Staff","Ship Staff Insp.","ME Jackte water cooler unable to maintain temp.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","ME jckt water cooler CIP carried out. Cooler heat exchange rate improved drastically","2021-07-23","","Completed","2021-07-05","No","No","No","Internal"]
[null,null,null,null,20124,"23_16/07/2021 9:26:45 PM","2021-06-17","Defect","Ship Staff","Ship Staff Insp.","High sea chest strainer found shifted from position.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","High sea chest strainer opening cut to match the intake, guides welded in place and strainer secured in position.","2021-07-15","","Completed","2021-06-30","No","No","No","Internal"]
[null,null,null,null,20119,"23_17/07/2021 10:29:36 AM","2021-06-20","Defect","Ship Staff","Ship Staff Insp.","Various valves in E/rm leaking","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Various leaking valves to be renewed in D/DOCK.","2021-09-30","DHAW210199","Completed","2021-11-27","Yes","No","No","Internal","RO still not in office DB- follow up in separate mail with procure in copy"]
[null,null,null,null,20125,"23_16/07/2021 5:41:48 PM","2021-06-20","Defect","Ship Staff","Ship Staff Insp.","ME unit #2 puncture valve found leaking.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Leaking punture valve replaced with overhauled spare.","2021-07-21","","Completed","2021-07-05","No","No","No","Internal"]
[null,null,null,null,20126,"23_16/07/2021 9:32:25 PM","2021-07-01","Defect","Ship Staff","Ship Staff Insp.","OWS throughput reduced.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Line filters cleaned.Coalescer element found completely chocked same was renewed. RO for the spare coalesecer element raised.","2021-07-10","","Completed","2021-07-04","No","No","No","Internal"]
[null,null,null,null,20123,"23_16/07/2021 3:54:14 PM","2021-07-06","Defect","Ship Staff","Ship Staff Insp.","Minor leak observed from #2 s.w service pump mechanical seal.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","","","","","Pump overhauled. Leakage stopped.","2021-09-30","DHAW210176","Completed","2021-11-22","No","No","No","Internal","RO  processed for supply. Follow up with purchase for the spares arrangements"]
[null,null,null,null,20120,"23_17/07/2021 9:51:35 AM","2021-07-13","Breakdown,Observation","Ship Staff","Ship Staff Insp.","Soft patch on deck seal overboard valve body in pump room bottom.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","2.9","Medium","","","Deck seal overboard valve renewed at singapore by plugging the overboard by diving team","2022-07-31","DHAW210217","Completed","2021-08-18","No","No","No","Internal","class approved  valve arranged at Singapore.\njob to be taken up along with propeller polishing at Singapore. - 12 Aug"]
[null,null,null,null,20121,"23_17/07/2021 9:53:07 AM","2021-07-13","Observation","Ship Staff","Ship Staff Insp.","Portside drip tray drain line has a soft patch near the welded portion to the drip tray","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","","","","","Refman entry made","2022-07-31","","Completed","2021-09-28","No","No","No","Internal","make repair spec in REFMAN and forward the export to office on priority. Repair specs not yet received"]
[null,null,null,null,20218,"23_24/07/2021 2:53:59 PM","2021-07-14","Observation","Ship Staff","Ship Staff Insp.","No 2 Cargo line leaking near 4C COT area due to worn out dresser coupling gasket during pressure testing","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.3","Very High","","","Dresser coupling gasket renewed & line again pressure tested to confirm integrity","2021-07-15","","Completed","2021-07-14","No","No","No","Internal"]
[null,null,null,null,20219,"23_24/07/2021 2:43:56 PM","2021-07-18","Observation","Ship Staff","Ship Staff Insp.","Stbd side accommodation ladder slewing motor found to be very slow","Deck - Machinery","General Appearance","Equipment Related","","","","","Motor overhauled. Vanes & bearing renewed. Motor tested & performance found enhanced & satisafactory","2021-07-31","","Completed","2021-07-20","No","No","No","Internal"]
[null,null,null,null,20213,"23_01/08/2021 6:52:13 PM","2021-07-19","Defect","Ship Staff","Ship Staff Insp.","Main Steam Inlet valve in pumproom for stripper pump leaking","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","","","","","Valves replaced and ok","2021-08-31","","Completed","2021-08-28","No","No","No","Internal","complete as planned prior arrival Singapore if possible and close out."]
[null,null,null,null,20220,"23_24/07/2021 2:41:25 PM","2021-07-20","Observation","Ship Staff","Ship Staff Insp.","Portside accommodation ladder hoisting & lowering air motor too slow & not able to lift the weight of the ladder","Deck - Machinery","General Appearance","Equipment Related","","","","","Overhauled the motor. Rotor vanes & Bearings renewed. Motor performance tested & observed to be enhanced.","2021-07-31","","Completed","2021-07-24","No","No","No","Internal"]
[null,null,null,null,20214,"23_01/08/2021 8:10:51 AM","2021-07-22","Defect","Ship Staff","Ship Staff Insp.","DG Inlet FO flowmeter internal leak.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.33","High","","","Job deferred to D/D. PO DHAW210221.","2021-09-21","DHAW210221 ","Completed","2021-11-27","Yes","No","No","Internal","processed for supply, follow up with procure"]
[null,null,null,null,20215,"23_29/07/2021 9:23:36 AM","2021-07-28","Defect","Ship Staff","Ship Staff Insp.","ECR and main switchboard AC SW cooling pipes corrosion noted.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.34","High","","","New pipes fabricated and fitted in place.","2022-05-31","","Completed","2021-11-18","No","No","No","Internal","kindly complete the job as discussed and close out.\nadditional repair specs to be made in DDRL  for replacing with galvanised pipes"]
[null,null,null,null,20221,"23_30/07/2021 10:36:41 AM","2021-07-28","Breakdown,Non Conformity,Observation","Ship Staff","Ship Staff Insp.","Cargo tank over fill alarm air horn faulty","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.14","Very High","","","Solenoid for the horn found stuck, same removed from place and overhauled. Solenoid fitted back in place. Horn tried out","2021-08-30","","Completed","2021-08-01","No","No","No","Internal"]
[null,null,null,null,20217,"23_31/07/2021 6:54:30 PM","2021-07-29","Observation","Ship Staff","Ship Staff Insp.","Deck scupper ovbd line in E/rm leak noted.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Overboard plugged and both valves renewed. Pipe section removed from place and repairs by welding carried out. Jig fabricated for the same. Pipe fabrication in progress.","2021-10-01","DHAW210266","Completed","2021-09-28","No","No","No","Internal","complete as planned and close out. Diving team arranged and the spare valve will be supplied for replacement this call at Singapore"]
[null,null,null,null,15415,"23_29/11/2020 9:15:56 PM","2021-07-31","Defect","Ship Staff","Ship Staff Insp.","No 2 general sea water pump poor performance and  to open up & check the condition of impeller & wear rings","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.31","Very High","","","Pump overhauled,now found satisfactory.","2021-11-01","DHAW210176","Completed","2021-11-24","No","No","No","Internal","Complete and close out as planned"]
[null,null,null,null,20521,"23_02/08/2021 3:32:06 PM","2021-08-02","Observation","Ship Staff","Ship Staff Insp.","Steam inlet valves for stripping pump in PR are leaking. require spares","E/R - Pipes/ valves & fittings","Cargo / Ballast Systems","Equipment Related","8.11","Medium","","","Require spares to replace the leaking valves","2021-09-10","DHAW210233","Completed","2021-08-28","No","No","No","Internal","valves connected at Singapore. kindly complete and close out"]
[null,null,null,null,20522,"23_04/08/2021 11:51:08 AM","2021-08-02","Observation","Ship Staff","Ship Staff Insp.","Intrinsic safe Pneumatic lamp for tank entry- Lamp was observed to have fused while testing","Miscellaneous","General Appearance","Equipment Related","","","","","Renewed the fused lamp. Equipment tested. Found satisfactory. Stored in mid ship locker","2021-09-10","DHAW210229","Completed","2021-09-09","No","No","No","Internal","confirm if the spares received at Singapore.\nclose out."]
[null,null,null,null,20527,"23_10/08/2021 8:10:05 AM","2021-08-02","Observation","Ship Staff","Ship Staff Insp.","3C COT stripping suction valve seat ring damage","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.11","Medium","","","Valve opened for inspection. Damaged seat ring renewed","2021-08-30","","Completed","2021-08-09","No","No","No","Internal"]
[null,null,null,null,20528,"23_10/08/2021 8:12:20 AM","2021-08-02","Observation","Ship Staff","Ship Staff Insp.","3P COT stripping suction valve found leaking","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.11","Medium","","","Valve opened & inspected. Seat ring found damaged. Same renewed","2021-08-30","","Completed","2021-08-09","No","No","No","Internal"]
[null,null,null,null,20529,"23_10/08/2021 8:13:56 AM","2021-08-02","Observation","Ship Staff","Ship Staff Insp.","4S COT stripping suction valve observed to be leaking","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.11","Medium","","","Valve opened for inspection. Damaged seat ring renewed","2021-08-30","","Completed","2021-08-09","No","No","No","Internal"]
[null,null,null,null,20530,"23_10/08/2021 8:16:20 AM","2021-08-02","Observation","Ship Staff","Ship Staff Insp.","Slop Stbd suction valve SRV 841 observed leaking ","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.11","Medium","","","Valve removed for inspection. Damaged seat ring renewed","2021-08-07","","Completed","2021-08-05","No","No","No","Internal"]
[null,null,null,null,20531,"23_10/08/2021 8:17:55 AM","2021-08-02","Observation","Ship Staff","Ship Staff Insp.","SRV 832 in PR observed to be leaking","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.11","Medium","","","Valve removed for inspection. Damaged seat ring renewed","2021-08-07","","Completed","2021-08-05","No","No","No","Internal"]
[null,null,null,null,20532,"23_10/08/2021 8:19:48 AM","2021-08-02","Observation","Ship Staff","Ship Staff Insp.","SRV 843- Cargo eductor suction valve observed to be leaking","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.11","Medium","","","Valve removed for inspection. Damaged seat ring renewed","2021-08-07","","Completed","2021-08-05","No","No","No","Internal"]
[null,null,null,null,20523,"23_14/08/2021 2:45:04 PM","2021-08-04","Observation","Ship Staff","Ship Staff Insp.","Draft gauges response too slow with change in draft during cargo operation. The draft gauges settles down to show correct reading after considerable time","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.13","Medium","","","All draft gauges over hauled. O-rings renewed. Air filter cleaned. Stbd side draft gauge renewed with brand new spare available onboard","2021-10-30","DHAW210267","Completed","2021-10-05","No","No","No","Internal","spares are arranged for supply this call. makers will provide remote assistance. follow up once the spares are received."]
[null,null,null,null,20533,"23_14/08/2021 2:40:51 PM","2021-08-04","Observation","Ship Staff","Ship Staff Insp.","AUS sealing tank drain valve found frozen","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.11","Medium","","","Valve overhauled. Proper working verfied and boxed up ","2021-08-30","","Completed","2021-08-13","No","No","No","Internal"]
[null,null,null,null,20525,"23_14/08/2021 10:51:28 AM","2021-08-13","Defect","Ship Staff","Ship Staff Insp.","STARBOARD WINDLASS FOUND OIL LEAK THROUGH CONTROL VALVE HANDLE SEALS.","Deck - Mooring Machinery","Mooring","Equipment Related","","","","","Control valve's sealing rings renewed.Leakage stopped.","2021-11-30","DHAW210251.","Completed","2021-11-16","No","No","No","Internal","spares to be arranged.\nvessel has one complete valve block- kindly replace with that for now."]
[null,null,null,null,20526,"23_14/08/2021 9:40:39 AM","2021-08-16","Observation","Ship Staff","Ship Staff Insp.","Mooring winch M10 leak noted between hydraulic motor and pipe","Deck - Mooring Machinery","Mooring","Equipment Related","1.3","Low","","","Pipe removed and O-ring renewed. Leak rectified","2021-08-30","","Completed","2021-08-28","No","No","No","Internal","complete as planned and close out"]
[null,null,null,null,20761,"23_23/08/2021 2:24:59 PM","2021-08-18","Observation","Ship Staff","Ship Staff Insp.","knob for ODME flow meter inlet flow valve found to be loose. Same to be tightened or replaced","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","","","","","Valve wheel replaced and the issue resolved","2021-09-15","","Completed","2021-08-25","No","No","No","Internal"]
[null,null,null,null,20747,"23_26/08/2021 11:24:56 AM","2021-08-19","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Boiler blowdown line to inspect for clogging.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.33","High","","","Boilers blowndown under pressure noted blowdown occuring with overboard getting hot and boilers water level dropping","2021-09-15","","Completed","2021-09-13","No","No","No","Internal"]
[null,null,null,null,20748,"23_26/08/2021 12:12:33 PM","2021-08-19","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","1.Paint over large areas on Main deck is cracking, there appears to be poor adhesion between the old red paint and new green coat. Starboard side Main deck between 1S and 3S is in poor condition and needs to be attended to. Forward areas on port side from forward to 3P also require cosmetic upgrade.","Hull & Tanks","General Appearance","Equipment Related","11.3","Medium","","","All areas on Main Deck having substantial corrosion/ flaking of paint derusted and painted with Primeer & deck Green. Spot derusting/ routine maintenance in progress.","2021-11-15","","Completed","2021-11-29","No","No","No","Internal","complete as planned and close out"]
[null,null,null,null,20749,"23_26/08/2021 12:14:38 PM","2021-08-19","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","2.Accommodation front and bridge wing support pillars are in below satisfactory condition and require cosmetic upgradation.","Hull & Tanks","General Appearance","Equipment Related","11.8","Low","","","De-rusting & painting of bridge wing supports & accommodation block carried out upto reachable limits","2021-12-30","","Completed","2021-11-24","No","No","No","Internal","complete as planned and close out"]
[null,null,null,null,20750,"23_26/08/2021 12:16:39 PM","2021-08-19","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","3. COV 511 - Noted to be leaking during last operation - seat ring to be renewed.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.11","Medium","","","Renewed the damaged seat ring of COV 511","2021-09-22","","Completed","2021-09-09","No","No","No","Internal"]
[null,null,null,null,20751,"23_26/08/2021 12:24:03 PM","2021-08-19","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","2. Deck seal u-pipe appears to have pitting corrosion - close up inspection to be carried out. ","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.44","High","","","Close up inspection carried out. No pitting. Area wire brushed & painted","2021-09-15","","Completed","2021-09-10","No","No","No","Internal"]
[null,null,null,null,20752,"23_26/08/2021 12:26:19 PM","2021-08-19","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","4. ODME Overboard blank, observed to have a crack, same to be opened up and inspected","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","","","","","ODME overboard blank removed & inspected. No cracks observed. Seal checked. In good condition. Same put back & the nuts & bolts tightned","2021-09-15","","Completed","2021-09-11","No","No","No","Internal"]
[null,null,null,null,20762,"23_26/08/2021 11:16:21 AM","2021-08-19","Observation","Ship Staff","Ship Staff Insp.","Port hose handling crane winching joy stick not returning to neutral position","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","11.3","Medium","","","Winch joy stick renewed with new spare","2021-09-03","","Completed","2021-08-25","No","No","No","Internal"]
[null,null,null,null,20763,"23_26/08/2021 11:19:49 AM","2021-08-19","Observation","Ship Staff","Ship Staff Insp.","Both HHCs wicnh limit switch housing cover to replace","Deck - Machinery","Cargo / Ballast Systems","Equipment Related","11.7","High","","","Both HHCs winch limit switch housing cover and gasket renewed.","2021-09-03","","Completed","2021-08-26","No","No","No","Internal"]
[null,null,null,null,20764,"23_26/08/2021 12:19:09 PM","2021-08-19","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","1. It was seen that all scupper plugs have cement as reinforcement - please confirm if all scuppers are sealing well. ","Deck - Pipe / Fittings","MARPOL Related","Equipment Related","","","","","All scuppers are sealing. Cement was put as an extra precaution","2021-08-21","","Completed","2021-08-20","No","No","No","Internal"]
[null,null,null,null,20765,"23_26/08/2021 12:30:37 PM","2021-08-19","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","3. Crew laundry House-keeping to be improved upon","Miscellaneous","General Appearance","Behaviour Based","11.14","Medium","","","Clean up crew laundry. Instruct all crew to keep the laundry clean & tidy at all times","2021-09-05","","Completed","2021-08-25","No","No","No","Internal"]
[null,null,null,null,20766,"23_26/08/2021 12:38:58 PM","2021-08-19","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","8.\tVessel had numerous spare hydraulic hoses for the hose handling crane, however there was no inventory or markings on the hoses to identify where the hoses would be utilized. An inventory of the hoses was also not available","Deck - Machinery","Cargo / Ballast Systems","Equipment Related","","","","","Inventory taken & onboard filing carried out","2021-09-25","","Completed","2021-08-24","No","No","No","Internal"]
[null,null,null,null,20767,"23_26/08/2021 12:34:36 PM","2021-08-19","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","4. During course of inspection a record of testing security communication equipment could not be sighted. (See attached Sample)","Miscellaneous","ISPS Related","Inappropriate Procedure","7.4","Low","","","New form made for records of testing of security equipments & filing carried out in ISPS log ","2021-08-26","","Completed","2021-08-25","No","No","No","Internal"]
[null,null,null,null,21594,"23_05/10/2021 5:26:26 PM","2021-08-19","Observation","Ship Staff","Ship Staff Insp.","E-deck stbd side alleyway door can not be closed as the door is damaged. ","Accommodation","General Appearance","Equipment Related","11.6","Medium","","","Replaced with new door and frame.","2021-11-30","","Completed","2021-11-29","No","No","No","Internal"]
[null,null,null,null,20753,"23_26/08/2021 11:31:38 AM","2021-08-20","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Air leak near Stbd boiler FD fan positioner control","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.3","Medium","","","Air leakage rectified.","2021-09-03","","Completed","2021-10-19","No","No","No","Internal","close out on priority please"]
[null,null,null,null,20754,"23_26/08/2021 11:38:16 AM","2021-08-25","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Both windlass and winches all the claw couplings to clean all the rust specially the coupling faces, apply light grease.","Deck - Mooring Machinery","Mooring","Equipment Related","11.3","Medium","","","Old grease removed and light grease applied to all claw coupling on windlass & winches","2021-09-25","","Completed","2021-09-05","No","No","No","Internal"]
[null,null,null,null,20755,"23_26/08/2021 11:54:18 AM","2021-08-25","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Stbd bridge wing bulkhead below ship name plate dirty.","Accommodation","General Appearance","Equipment Related","12.12","High","","","De-rusting & painting completed","2021-09-25","","Completed","2021-09-17","No","No","No","Internal","it is small job and at convenient location should have bein closed by now."]
[null,null,null,null,20756,"23_26/08/2021 11:56:03 AM","2021-08-25","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Spot Maintenance of MGO and HFO bunker lines required, specially bottom","Deck - Pipe / Fittings","General Appearance","Equipment Related","9.14","Medium","","","HFO/LSMGO bunker pipeline derusted,found in good condition. then painted.","2021-10-31","","Completed","2021-10-28","No","No","No","Internal","complete as planned and close out"]
[null,null,null,null,20757,"23_26/08/2021 11:59:54 AM","2021-08-25","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Arrange to dispose the old radar after consulting with electrical department.","Navigation - RADAR","General Appearance","Equipment Related","10.29","Medium","","","Off landed at Singapore with garbage LR55/2021","2021-09-30","","Completed","2021-09-28","No","No","No","Internal","complete as planned and close out"]
[null,null,null,null,20758,"23_26/08/2021 12:01:16 PM","2021-08-25","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Paint the spare kenster shackle and chain studs and stencil on bulkhead","Deck - Mooring Machinery","General Appearance","Equipment Related","12.2","High","","","Spare kenter shackle & chain studs painted and stored in fpk store","2021-09-25","","Completed","2021-09-04","No","No","No","Internal"]
[null,null,null,null,20759,"23_26/08/2021 12:04:43 PM","2021-08-25","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","One Pedestal rollers on P. forecastle need to adjust height as it is sitting on the bottom plate","Deck - Mooring Machinery","Mooring","Equipment Related","12.1","High","","","Proper working of the roller pedestal was verfied during loading operations at SPM. Plan to attend the same on completion of jobs at hand","2021-10-24","","Completed","2021-10-30","No","No","No","Internal","complete as planned and close out"]
[null,null,null,null,20760,"23_26/08/2021 11:41:31 AM","2021-08-25","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Both life boat davit wires end not correctly secured in the wedge. The loaded part of wire has to be in straight part of the wedge.","LSA / FFA","Safety / LSA / FFA","Inappropriate Procedure","8.5","Very High","","","Wire direction changed. Lifeboat tested by lowering to embarkation deck. All ok","2021-10-25","","Completed","2021-09-18","No","No","No","Internal","complete as planned and close out"]
[null,null,null,null,20768,"23_26/08/2021 12:02:58 PM","2021-08-25","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","AUS pump unit one minor drip leak from thin line.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","10.32","Very High","","","Repaired the leak from AUS motor to pressure gauge fitted in PR top.","2021-09-10","","Completed","2021-08-28","No","No","No","Internal"]
[null,null,null,null,20769,"23_26/08/2021 11:57:54 AM","2021-08-25","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Bridge wing broken rubber mats pieces to be discarded","Accommodation","General Appearance","Equipment Related","12.12","High","","","Broken rubber mats discarded in garbage","2021-09-05","","Completed","2021-08-28","No","No","No","Internal"]
[null,null,null,null,21346,"23_02/10/2021 5:02:42 PM","2021-08-25","Defect","Ship Staff","Ship Staff Insp.","Atmospheric condensor compensator leak to be rectified","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.34","High","","","Atmospheric condensor-stm condensate return line pipe fabricated and fitted in place.","2021-11-30","","Completed","2021-11-11","No","No","No","Internal"]
[null,null,null,null,21596,"23_04/10/2021 1:41:53 PM","2021-08-27","Observation","Ship Staff","Ship Staff Insp.","Repair the emergency generator air inlet door & it's channel for rubber packing on C-deck aft","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.6","Medium","","","Repaired the wasted lips and eyes of the air inlet door","2021-12-30","","Completed","2021-10-30","No","No","No","Internal","try and complete before Nov End."]
[null,null,null,null,20770,"23_02/09/2021 1:38:31 PM","2021-08-28","Observation","Ship Staff","Ship Staff Insp.","Galley oven door closing arrangement to be repaired as the rivets holding them broke off","Miscellaneous","General Appearance","Equipment Related","","","","","Riveting of the closing arrangement red-done. Confirmed proper locking of galley oven door","2021-08-31","","Completed","2021-08-31","No","No","No","Internal"]
[null,null,null,null,21109,"23_11/09/2021 10:18:30 AM","2021-09-08","Observation","Ship Staff","Ship Staff Insp.","Deck air line near 2C COT found leaking ","Deck - Pipe / Fittings","General Appearance","Equipment Related","8.44","High","","","Leaking section removed to ER work shop & repaired the leak","2021-09-10","","Completed","2021-09-09","No","No","No","Internal"]
[null,null,null,null,21110,"23_14/09/2021 5:54:04 PM","2021-09-08","Defect","Ship Staff","Ship Staff Insp.","Aux boiler feed pump NO 1 anti overheating orifice leaking","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.33","High","","","Antiheating orifice leak rectified, DHAW210262 raised for additional spare","2021-09-20","DHAW210262","Completed","2021-09-13","No","No","No","Internal"]
[null,null,null,null,21111,"23_14/09/2021 5:57:37 PM","2021-09-08","Defect","Ship Staff","Ship Staff Insp.","Aux boiler feed pump NO 2 leak noted from fwd cover gasket/seal.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.33","High","","","FWD gasket cover found loose, same tightened and leak rectified.","2021-09-17","","Completed","2021-09-14","No","No","No","Internal"]
[null,null,null,null,21601,"23_04/10/2021 2:54:01 PM","2021-09-17","Breakdown","Ship Staff","Ship Staff Insp.","Aux boiler feed pump #2, tripping. Cuase to be investigated and rectified","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.34","High","","","Pump dismantled,noticed Stage piece was wrong spare part, same replaced by one old and new spare parts.suspect previous alignment with motor.Now,pump assembled and fitted in place,then tried out-found working satisfactorily.","2021-10-15","","Completed","2021-10-15","No","No","No","Internal"]
[null,null,null,null,21347,"23_29/09/2021 3:59:19 PM","2021-09-25","Observation","Ship Staff","Ship Staff Insp.","AUS fresh water tank to slop port gas extraction pipe holed. The pipe can not be removed to work shop for repair as one of the pipe is welded to AUS freshwater tank it self.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.44","High","","","Soft repair carried out with devcon. Leak arrested. The pipe is not subject to high pressure. Permanent repair to be carried out in drydock. Entry made in Refman","2022-08-30","","Completed","2021-10-04","No","No","No","Internal","kindly forward the refman export and close out under DDRL."]
[null,null,null,null,null,"23_05/10/2021 5:25:18 PM","2021-09-26","Observation","Ship Staff","Ship Staff Insp.","C-deck stbd side alleyway door is hard to close.","Accommodation","General Appearance","Equipment Related",11.6,"Medium","Not Applicable","Not Applicable","New spare door is not the same size and cannot be fitted. New order to be placed or in DD. Defect transferred to REFMAN for DD repairs.","2021-12-31",null,"Completed","2021-12-30","No",null,null,"Internal"]
[null,null,null,null,21597,"23_04/10/2021 1:44:19 PM","2021-09-28","Observation","Ship Staff","Ship Staff Insp.","Repair the leak on stbd side gangway pneumatic line near control box","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.4","Very High","","","Renewed the line and tried out, satisfactory operation","2021-11-30","","Completed","2021-10-26","No","No","No","Internal","complete and close out as planned"]
[null,null,null,null,21350,"23_01/10/2021 11:49:12 AM","2021-09-30","Observation","Ship Staff","Ship Staff Insp.","Provision crane safety limit switch broken and not in place.","Deck - Machinery","ISM Related","Equipment Related","8.5","Very High","","","Refited the limit switch of provision crane","2021-10-04","","Completed","2021-10-02","No","No","No","Internal"]
[null,null,null,null,21602,"23_05/10/2021 5:49:57 PM","2021-10-02","Observation","Ship Staff","Ship Staff Insp.","Renew the rubber packing of Bosun store entrance door","Miscellaneous","General Appearance","Equipment Related","11.6","Medium","","","Renewed with the new rubber packing","2021-10-30","","Completed","2021-10-07","No","No","No","Internal"]
[null,null,null,null,21603,"23_05/10/2021 5:48:25 PM","2021-10-02","Observation","Ship Staff","Ship Staff Insp.","Renew the rubber packing of mid ship locker","Miscellaneous","General Appearance","Equipment Related","11.6","Medium","","","Renewed with the new rubber packing ","2021-10-30","","Completed","2021-10-05","No","No","No","Internal"]
[null,null,null,null,21349,"23_02/10/2021 5:11:48 PM","2021-10-02","Defect","Ship Staff","Ship Staff Insp.","ME unit #1 fuel pump steel pipe developed hole.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.34","High","","","ME unit #1 fuel pump pipe developed hole. Pipe repaired by welding.","2021-10-30","","Completed","2021-10-21","No","No","No","Internal","carry out repairs at the earliest and close out"]
[null,null,null,null,21600,"23_04/10/2021 1:34:19 PM","2021-10-04","Observation","Ship Staff","Ship Staff Insp.","Pin hole leak from 1S COT manhole cover gas sampling point while de-rusting of the same. Soft repair carried out","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.12","Medium","","","repaired and fitted back","2021-11-02","","Completed","2021-10-19","No","No","No","Internal","complete as planned and close out"]
[null,null,null,null,22004,"23_22-Oct-21 14:31:43","2021-10-19","Observation","Ship Staff","Ship Staff Insp.","X-Band Radar JRC JMR9225, showing alarm-\"Life expectancy TX/RX 1 fan at all times.","Navigation - RADAR","Navigation","Equipment Related","4.7","High","","","Being followed up with Navcom support.","2021-11-19","","Completed","2021-10-26","No","No","No","Internal","to be done during the next routine serv. automated alarm"]
[null,null,null,null,22005,"23_22-Oct-21 14:45:21","2021-10-19","Observation","Ship Staff","Ship Staff Insp.","No.2 DGPS Furuno GP170, showing alarm \"loss of differential signal\" at all times, however No1 DGPS doesnot have this alarm. Same cannot be reset.","Navigation - DGPS / EPFS / AIS","Navigation","Equipment Related","4.7","High","","","System switched off and on and alarm was reset.","2021-11-19","","Completed","2021-10-24","No","No","No","Internal"]
[null,null,null,null,22006,"23_22-Oct-21 14:47:11","2021-10-19","Observation","Ship Staff","Ship Staff Insp.","Speed log Furuno DS30; date is showing incorrect as in its setting Year cannot be changed beyond 2020","Navigation - Echo Sounder / Speed Log","Navigation","Equipment Related","4.7","High","","","Date changed, year input 2021","2021-11-19","","Completed","2021-10-24","No","No","No","Internal","corresponded and remote trouble shooting is arranged"]
[null,null,null,null,22008,"23_22-Oct-21 14:53:20","2021-10-19","Observation","Ship Staff","Ship Staff Insp.","Fire detection repeater panel (Tycomarine T1232-C),  in Fire station found disconnected. ","Miscellaneous","Emgcy. Systems","Human Error","5.35","Medium","","","Fire detection repeater panel found disconnected due to false alarm, same connected back,no alarm exists.","2021-11-19","","Completed","2021-11-18","No","No","No","Internal"]
[null,null,null,null,22009,"23_22/10/2021 10:35:45 PM","2021-10-20","Defect","Ship Staff","Ship Staff Insp.","COP emergency trip mounting at Pump room entrance has corroded and come loose from the bracket and is tied with rope.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.8","Medium","","","Repaired and fitted back","2021-11-20","","Completed","2021-10-26","No","No","No","Internal","complete as planned and close out"]
[null,null,null,null,22011,"23_22/10/2021 10:47:33 PM","2021-10-20","Observation","Ship Staff","Ship Staff Insp.","Deck steam line to Slop stbd. tank is heated/ pressurized as Isolation V/V in E/R not holding.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.11","Medium","","","Job deferred to d/dock. Leaking valve to be overhauled.","2021-11-30","","Completed","2021-11-27","Yes","No","No","Internal","Raise RO for valve if unable to repair. Complete as planned and close out."]
[null,null,null,null,22013,"23_23/10/2021 10:52:56 AM","2021-10-20","Observation","Ship Staff","Ship Staff Insp.","One COW machine on Stbd. Slop and one on 4P COT are frozen and cannot be turned.","Cargo Mach.,Deck - Machinery","Cargo / Ballast Systems","Equipment Related","8.34","High","","","Overhauled and turning now.","2021-11-30","","Completed","2021-10-27","No","No","No","Internal","complete as planned and close out."]
[null,null,null,null,null,"23_22/10/2021 10:44:50 PM","2021-10-20","Breakdown","Ship Staff","Ship Staff Insp.","4S WBTgauge not working.","Hull & Tanks","Cargo / Ballast Systems","Equipment Related",8.8000000000000007,"Medium","Not Applicable","Not Applicable","unit purged and leak rectified, working satisfactory","2021-12-15",null,"Completed","2021-12-13","No",null,null,"Internal"]
[null,null,null,null,null,"23_22/10/2021 10:58:55 PM","2021-10-20","Observation","Ship Staff","Ship Staff Insp.","5PIG sensor is showing 130 mmWg higher value than actual; as compared to other tanks.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related",8.8000000000000007,"Medium","Not Applicable","Not Applicable","Sensor opened to atmoshphere and calibrated.","2021-12-31","DHAW210257","Completed","2021-12-14","No",null,null,"Internal"]

{"sheet":"Calc","index":2,"n_rows":28,"n_cols":12,"rows_kept":28,"cut":false,"hidden":true,"merged":[]}
["Def_type","Def_cause","Equipments","VIQrefno","Observer_code"]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,"Dim itemSele As Long"]
[null,null,null,null,null,null,null,null,null,null,null,"   dim startRow as integer"]
[null,null,null,null,null,null,null,null,null,null,null,"   startRow=1"]
[null,null,null,null,null,null,null,null,null,null,null,"        For itemSele = 0 To ListBox1.ListCount - 1"]
[null,null,null,null,null,null,null,null,null,null,null,"        If ListBox1.Selected(itemSele) = True Then"]
[null,null,null,null,null,null,null,null,null,null,null,"        Worksheets(\"WorksheetName\").Range(\"A\" & startRow).Value = ListBox1.List(itemSele)"]
[null,null,null,null,null,null,null,null,null,null,null,"        startRow = startRow + 1"]
[null,null,null,null,null,null,null,null,null,null,null,"        End If"]
[null,null,null,null,null,null,null,null,null,null,null,"        Next"]
[null,null,null,null,null,null,null,null,null,null,null,"Dim LastRowA As String"]
[null,null,null,null,null,null,null,null,null,null,null,"        Dim itemSele As Long"]
[null,null,null,null,null,null,null,null,null,null,null,"       Dim startRow as integer"]
[null,null,null,null,null,null,null,null,null,null,null,"        LastRowA = ActiveSheet.Cells(Rows.count, \"A\").End(xlUp).row"]
[null,null,null,null,null,null,null,null,null,null,null,"        startQue = 0"]
[null,null,null,null,null,null,null,null,null,null,null,"        For itemSele = 0 To ListBox1.ListCount - 1"]
[null,null,null,null,null,null,null,null,null,null,null,"        For startRow = 1 To LastRowA"]
[null,null,null,null,null,null,null,null,null,null,null,"        If Worksheets(\"WorksheetName\").Range(\"A\" & startRow).Value = ListBox1.List(itemSele) Then"]
[null,null,null,null,null,null,null,null,null,null,null,"        ListBox1.Selected(itemSele) = True"]
[null,null,null,null,null,null,null,null,null,null,null,"        Exit For"]
[null,null,null,null,null,null,null,null,null,null,null,"        End If"]
[null,null,null,null,null,null,null,null,null,null,null,"        Next j"]
[null,null,null,null,null,null,null,null,null,null,null,"        Next"]
[null,null,null,null,null,null,null,null,null,null,null,"        End If"]

{"sheet":"Areaofobs","index":3,"n_rows":17,"n_cols":2,"rows_kept":17,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Cargo / Ballast Systems",11]
["Cert. & Docu.",2]
["Communication",6]
["Crew Management",3]
["Emgcy. Systems",13]
["Eng. / Strg. Comp.",14]
["General Appearance",15]
["Ice Opns.",17]
["ISM Related",7]
["ISPS Related",10]
["MARPOL Related",9]
["MLC Related",4]
["Mooring",12]
["Navigation",5]
["Safety / LSA / FFA",8]
["Structural Condn. / WT integrity ",16]

{"sheet":"Vessel_type","index":4,"n_rows":1,"n_cols":2,"rows_kept":1,"cut":false,"hidden":true,"merged":[]}
["Vessel_type","ID"]

{"sheet":"Deficiency_type","index":5,"n_rows":8,"n_cols":3,"rows_kept":8,"cut":false,"hidden":true,"merged":[]}
["TITLE","Type of deficiency_description","ID"]
["Breakdown",null,6]
["Critical Equipment",null,4]
["Defect",null,1]
["Guarantee Claim",null,8]
["Non Conformity",null,2]
["Observation",null,3]
["Other",null,7]

{"sheet":"VIQrefno","index":6,"n_rows":427,"n_cols":3,"rows_kept":427,"cut":false,"hidden":true,"merged":[]}
["VIQ_ref_no","Risk Value of observation","ID"]
["1.1","Low",8243]
["1.10","Low",8252]
["1.11","Low",8253]
["1.12","Low",8254]
["1.13","Low",8255]
["1.14","Low",8256]
["1.15","Low",8257]
["1.16","Low",8259]
["1.17","Low",8260]
["1.18","Low",8261]
["1.19","Low",8262]
["1.2","Low",8244]
["1.20","Low",8263]
["1.21","Low",8265]
["1.22","Low",8266]
["1.23","Low",8267]
["1.24","Low",8268]
["1.25","Low",8269]
["1.26","Low",8270]
["1.3","Low",8245]
["1.4","Low",8246]
["1.5","Low",8247]
["1.6","Low",8248]
["1.7","Low",8249]
["1.8","Low",8250]
["1.9","Low",8251]
["1.99","High",11258]
["10.1","Medium",8461]
["10.10","High",8470]
["10.11","Medium",8471]
["10.12","Very High",8472]
["10.13","Very High",8473]
["10.14","Medium",8474]
["10.15","Low",8475]
["10.16","Very High",8476]
["10.17","Very High",8477]
["10.18","High",8478]
["10.19","Very High",8479]
["10.2","Low",8462]
["10.20","High",8480]
["10.21","Medium",8481]
["10.22","Low",8482]
["10.23","Medium",8483]
["10.24","Low",8484]
["10.25","Very High",8485]
["10.26","High",8486]
["10.27","Medium",8487]
["10.28","Low",8488]
["10.29","Medium",8489]
["10.3","Medium",8463]
["10.30","High",8490]
["10.31","Very High",8491]
["10.32","Very High",8492]
["10.33","High",8493]
["10.34","High",8494]
["10.35","Very High",8495]
["10.36","Very High",8496]
["10.37","Medium",8497]
["10.38","Medium",8498]
["10.39","High",8499]
["10.4","High",8464]
["10.40","Medium",8500]
["10.41","Medium",8501]
["10.42","Medium",8502]
["10.43","Medium",8503]
["10.44","Medium",8504]
["10.45","Very High",8505]
["10.46","High",8506]
["10.47","Medium",8507]
["10.48","High",8508]
["10.49","Medium",8509]
["10.5","Low",8465]
["10.50","High",8510]
["10.51","Low",8511]
["10.52","Medium",8512]
["10.53","Medium",8513]
["10.54","High",8514]
["10.55","Low",8515]
["10.6","Very High",8466]
["10.7","Medium",8467]
["10.8","Medium",8468]
["10.9","Medium",8469]
["10.99","High",8516]
["11.1","High",8420]
["11.10","Medium",8429]
["11.11","Very High",8430]
["11.12","Low",8431]
["11.13","Low",8432]
["11.14","Medium",8433]
["11.15","Low",8434]
["11.16","Low",8435]
["11.17","Low",8436]
["11.2","Medium",8421]
["11.3","Medium",8422]
["11.4","Very High",8423]
["11.5","Medium",8424]
["11.6","Medium",8425]
["11.7","High",8426]
["11.8","Low",8427]
["11.9","Low",8428]
["11.99","High",8437]
["12.1","High",8438]
["12.10","High",8448]
["12.11","High",8449]
["12.12","High",8450]
["12.13","High",8451]
["12.14","High",8452]
["12.15","High",8453]
["12.16","High",8454]
["12.17","High",8455]
["12.18","High",8456]
["12.19","High",8457]
["12.2","High",8439]
["12.20","High",8458]
["12.21","High",8459]
["12.3","High",8441]
["12.4","High",8442]
["12.5","High",8443]
["12.6","High",8444]
["12.7","High",8445]
["12.8","High",8446]
["12.9","High",8447]
["12.99","High",8460]
["2.1","Very High",8296]
["2.1.9","Very High",11259]
["2.10","Medium",8304]
["2.11","Medium",8305]
["2.12","Low",8306]
["2.13","Low",8307]
["2.14","Low",8308]
["2.15","Low",8309]
["2.16","Medium",8310]
["2.2","Medium",8297]
["2.3","High",8295]
["2.4","Medium",8298]
["2.5","Medium",8299]
["2.6","Low",8300]
["2.7","High",8301]
["2.8","High",8302]
["2.9","Medium",8303]
["2.99","High",8311]
["3.1","High",8312]
["3.2","Very High",8313]
["3.3","High",8314]
["3.4","Low",8294]
["3.5","Medium",8315]
["3.6","High",8316]
["3.7","Very High",8317]
["3.8","Very High",8318]
["3.99","High",8319]
["4.1","High",8320]
["4.10","High",8329]
["4.11","Medium",8330]
["4.12","Very High",8331]
["4.13","Very High",8332]
["4.14","Very High",8333]
["4.15","Very High",8334]
["4.16","Very High",8335]
["4.17","Very High",8336]
["4.18","Very High",8337]
["4.19","Low",8338]
["4.2","Medium",8321]
["4.20","Very High",8339]
["4.21","High",8340]
["4.22","Low",8341]
["4.23","High",8342]
["4.24","High",8343]
["4.25","Low",8344]
["4.26","Low",8345]
["4.27","High",8346]
["4.3","Medium",8322]
["4.4","High",8323]
["4.5","Very High",8324]
["4.6","Medium",8325]
["4.7","High",8326]
["4.8","Medium",8327]
["4.9","Medium",8328]
["4.99","High",8347]
["5.1","Very High",8517]
["5.10","High",8526]
["5.11","Low",8527]
["5.12","Medium",8528]
["5.13","High",8529]
["5.14","Very High",8530]
["5.15","Medium",8531]
["5.16","Very High",8532]
["5.17","Very High",8533]
["5.18","High",8534]
["5.19","Medium",8535]
["5.2","Very High",8518]
["5.20","Medium",8536]
["5.21","Medium",8537]
["5.22","High",8539]
["5.23","Very High",8540]
["5.24","Very High",8541]
["5.25","Medium",8542]
["5.26","Medium",8543]
["5.27","Medium",8544]
["5.28","Very High",8545]
["5.29","High",8546]
["5.3","Low",8519]
["5.30","High",8547]
["5.31","High",8548]
["5.32","High",8549]
["5.33","High",8550]
["5.34","Low",8551]
["5.35","Medium",8552]
["5.36","Low",8553]
["5.37","Low",8554]
["5.38","High",8555]
["5.39","Very High",8556]
["5.4","High",8520]
["5.40","Very High",8557]
["5.41","Very High",8558]
["5.42","Medium",8559]
["5.43","High",8560]
["5.44","High",8561]
["5.45","Medium",8564]
["5.46","Medium",8565]
["5.47","Medium",8566]
["5.48","Medium",8567]
["5.5","Low",8521]
["5.6","Low",8522]
["5.7","Medium",8523]
["5.8","Medium",8524]
["5.9","Very High",8525]
["5.99","High",8568]
["6.1","Medium",8348]
["6.10","Low",8357]
["6.11","High",8358]
["6.12","Medium",8359]
["6.13","Low",8360]
["6.14","High",8361]
["6.15","High",8362]
["6.16","Very High",8363]
["6.17","Very High",8364]
["6.18","Medium",8365]
["6.19","Low",8366]
["6.2","High",8349]
["6.20","Medium",8367]
["6.21","High",8368]
["6.22","Medium",8369]
["6.3","Low",8350]
["6.4","High",8351]
["6.5","Medium",8352]
["6.6","Medium",8353]
["6.7","High",8354]
["6.8","High",8355]
["6.9","Low",8356]
["6.99","High",8370]
["7.1","High",8371]
["7.10","High",8380]
["7.11","High",8381]
["7.12","High",8382]
["7.13","Medium",8383]
["7.14","Medium",8384]
["7.15","High",8385]
["7.16","High",8386]
["7.17","High",8387]
["7.2","High",8372]
["7.3","Low",8373]
["7.4","Low",8374]
["7.5","Low",8375]
["7.6","Medium",8376]
["7.7","Low",8377]
["7.8","High",8378]
["7.9","High",8379]
["7.99","High",8388]
["8.1","Very High",8569]
["8.10","Very High",8578]
["8.100","Low",11227]
["8.101","Medium",11228]
["8.102","Low",11229]
["8.103","Low",11230]
["8.104","Low",11231]
["8.105","Medium",11232]
["8.106","Medium",11233]
["8.107","Low",11234]
["8.108","High",11235]
["8.109","Very High",11236]
["8.11","Medium",8579]
["8.110","High",11237]
["8.111","Medium",11238]
["8.112","High",11239]
["8.113","Medium",11240]
["8.114","Low",11241]
["8.115","High",11242]
["8.116","Medium",11243]
["8.117","Medium",11244]
["8.118","Medium",11245]
["8.119","High",11246]
["8.12","Medium",8580]
["8.120","High",11247]
["8.121","Medium",11248]
["8.122","High",11249]
["8.123","High",11250]
["8.124","Low",11251]
["8.125","High",11252]
["8.126","Medium",11253]
["8.127","Medium",11254]
["8.13","Medium",8581]
["8.14","Very High",8582]
["8.15","High",8583]
["8.16","Very High",8584]
["8.17","Low",8585]
["8.18","High",8586]
["8.19","High",8587]
["8.199","High",11255]
["8.2","Medium",8570]
["8.20","Medium",8588]
["8.21","High",8589]
["8.22","Very High",8590]
["8.23","Medium",8591]
["8.24","Medium",8592]
["8.25","Very High",8593]
["8.26","High",8594]
["8.27","Medium",8595]
["8.28","Medium",8596]
["8.29","High",8598]
["8.3","Very High",8571]
["8.30","High",8599]
["8.31","High",8600]
["8.32","Low",8601]
["8.33","Medium",8602]
["8.34","High",8603]
["8.35","Medium",8604]
["8.36","Medium",8605]
["8.37","High",8607]
["8.38","Medium",8608]
["8.39","Medium",8609]
["8.4","Medium",8572]
["8.40","High",8610]
["8.41","Medium",8611]
["8.42","Medium",8612]
["8.43","Very High",8613]
["8.44","High",8615]
["8.45","High",8616]
["8.46","Very High",8617]
["8.47","Very High",8618]
["8.48","Medium",8619]
["8.49","High",8620]
["8.5","Very High",8573]
["8.50","Medium",8621]
["8.51","Low",8622]
["8.52","Low",8623]
["8.53","Low",8624]
["8.54","High",8625]
["8.55","Low",11182]
["8.56","Medium",11183]
["8.57","Medium",11184]
["8.58","High",11185]
["8.59","High",11186]
["8.6","Medium",8574]
["8.60","High",11187]
["8.61","Medium",11188]
["8.62","Very High",11189]
["8.63","High",11190]
["8.64","Medium",11191]
["8.65","Low",11192]
["8.66","High",11193]
["8.67","High",11194]
["8.68","High",11195]
["8.69","Medium",11196]
["8.7","High",8575]
["8.70","Medium",11197]
["8.71","Very High",11198]
["8.72","Medium",11199]
["8.73","Medium",11200]
["8.74","High",11201]
["8.75","Medium",11202]
["8.76","Medium",11203]
["8.77","Medium",11204]
["8.78","Medium",11205]
["8.79","Medium",11206]
["8.8","Medium",8576]
["8.80","Medium",11207]
["8.81","Low",11208]
["8.82","Medium",11209]
["8.83","Low",11210]
["8.84","Low",11211]
["8.85","Medium",11212]
["8.86","Medium",11213]
["8.87","Medium",11214]
["8.88","Low",11215]
["8.89","High",11216]
["8.9","High",8577]
["8.90","High",11217]
["8.91","High",11218]
["8.92","Medium",11219]
["8.93","Low",11220]
["8.94","Low",11221]
["8.95","Medium",11222]
["8.96","Medium",11223]
["8.97","Low",11224]
["8.98","High",11225]
["8.99","Medium",11226]
["9.1","Low",8390]
["9.10","Medium",8399]
["9.11","Medium",8400]
["9.12","Medium",8401]
["9.13","Low",8402]
["9.14","Medium",8403]
["9.15","Medium",8404]
["9.16","High",8405]
["9.17","High",8406]
["9.18","Low",8407]
["9.19","Low",8408]
["9.2","Very High",8391]
["9.20","Medium",8409]
["9.21","Medium",8410]
["9.22","Low",8411]
["9.23","Low",8412]
["9.24","Medium",8413]
["9.25","Low",8414]
["9.26","Low",8415]
["9.27","Low",8416]
["9.28","Medium",8417]
["9.29","Low",8418]
["9.3","Very High",8392]
["9.4","High",8393]
["9.5","High",8394]
["9.6","Low",8395]
["9.7","Medium",8396]
["9.8","Medium",8397]
["9.9","Medium",8398]
["9.99","High",8419]

{"sheet":"Equipment_list","index":7,"n_rows":28,"n_cols":3,"rows_kept":28,"cut":false,"hidden":true,"merged":[]}
["TITLE","Equipment_list_description","ID"]
["Accommodation",null,12]
["Cargo Mach.",null,13]
["Critical Equip.",null,16]
["Deck - Machinery",null,18]
["Deck - Mooring Machinery",null,15]
["Deck - Pipe / Fittings",null,20]
["Documentation",null,21]
["E/R - Air Comp.",null,8]
["E/R - Aux. Engine",null,4]
["E/R - Aux. Mach.",null,7]
["E/R - Boiler",null,5]
["E/R - Main Engine",null,3]
["E/R - Pipes/ valves & fittings",null,9]
["E/R - Pumps",null,32]
["E/R - Purifier",null,6]
["Elect. Mach. & Equip.",null,10]
["Hull & Tanks",null,19]
["Inert Gas",null,14]
["LSA / FFA",null,17]
["Miscellaneous",null,22]
["Navigation - DGPS / EPFS / AIS",null,28]
["Navigation - ECDIS",null,25]
["Navigation - Echo Sounder / Speed Log",null,26]
["Navigation - GMDSS & Communication",null,23]
["Navigation - Others",null,11]
["Navigation - RADAR",null,24]
["Navigation - VDR / BNWAS",null,30]

{"sheet":"PSC_MOU","index":8,"n_rows":11,"n_cols":3,"rows_kept":11,"cut":false,"hidden":true,"merged":[]}
["TITLE","PSC_MOU_description","ID"]
["Asia and the Pacific",null,2]
["Caribbean",null,4]
["Europe and the North Atlantic",null,1]
["Latin America",null,3]
["The Black Sea region",null,6]
["The Indian Ocean",null,8]
["The Mediterranean",null,7]
["The Riyadh MoU",null,9]
["USCG",null,10]
["West and Central Africa",null,5]

{"sheet":"Inspection_type","index":9,"n_rows":13,"n_cols":2,"rows_kept":13,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Bunkering Audit",14]
["Cargo Audit",17]
["Engineering Audit",16]
["ISM Audit",2]
["ISPS Audit",3]
["IT Audit",10]
["MLC Audit",1]
["Mooring Audit",9]
["Nav Audit / Verification",8]
["Onboard Training",18]
["Ship Staff Insp.",15]
["Suptd. Insp.",13]

{"sheet":"Deficiency_Cause","index":10,"n_rows":8,"n_cols":3,"rows_kept":8,"cut":false,"hidden":true,"merged":[]}
["TITLE","Deficiency_Cause_description","ID"]
["Behaviour Based",null,1]
["Equipment Related",null,4]
["External Factors",null,5]
["Human Error",null,7]
["Inappropriate Procedure",null,8]
["Industry Issue",null,6]
["Knowledge Based",null,3]

{"sheet":"Observer_code","index":11,"n_rows":3,"n_cols":3,"rows_kept":3,"cut":false,"hidden":true,"merged":[]}
["TITLE","Observer_code_description","ID"]
["Owner / Marine / Tech. Suptd.",null,3]
["Ship Staff",null,2]

{"sheet":"Status_code","index":12,"n_rows":6,"n_cols":3,"rows_kept":6,"cut":false,"hidden":true,"merged":[]}
["TITLE","Status_code_description","ID"]
["Completed",null,6]
["Deferred to D D",null,5]
["In progress",null,3]
["Not Started",null,2]
["Waiting spare",null,4]

{"sheet":"PSC_ref_no","index":13,"n_rows":19,"n_cols":2,"rows_kept":19,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Alarms",9]
["Cargo operations including equipment",7]
["Certificates & Documentation",2]
["Dangerous Goods",13]
["Emergency Systems",5]
["Fire safety",8]
["ISM",16]
["ISPS",17]
["Life saving appliances",12]
["MLC, 2006",18]
["Other",19]
["Pollution Prevention",15]
["Propulsion and auxiliary machinery",14]
["Radio communication",6]
["Safety of Navigation",11]
["Structural condition",3]
["Water/Weathertight condition",4]
["Working and Living Conditions",10]

{"sheet":"Risk_value_of_obs","index":14,"n_rows":1,"n_cols":2,"rows_kept":1,"cut":false,"hidden":true,"merged":[]}
["Risk Value of observation","ID"]

{"sheet":"Year","index":15,"n_rows":18,"n_cols":1,"rows_kept":18,"cut":false,"hidden":true,"merged":[]}
["Year"]
[2014]
[2015]
[2016]
[2017]
[2018]
[2019]
[2020]
[2021]
[2022]
[2023]
[2024]
[2025]
[2026]
[2027]
[2028]
[2029]
[2030]

{"sheet":"Month","index":16,"n_rows":13,"n_cols":1,"rows_kept":13,"cut":false,"hidden":true,"merged":[]}
["Month"]
["Jan"]
["Feb"]
["Mar"]
["Apr"]
["May"]
["Jun"]
["Jul"]
["Aug"]
["Sep"]
["Oct"]
["Nov"]
["Dec"]

{"sheet":"Date_","index":17,"n_rows":32,"n_cols":1,"rows_kept":32,"cut":false,"hidden":true,"merged":[]}
["Date"]
["01"]
["02"]
["03"]
["04"]
["05"]
["06"]
["07"]
["08"]
["09"]
[10]
[11]
[12]
[13]
[14]
[15]
[16]
[17]
[18]
[19]
[20]
[21]
[22]
[23]
[24]
[25]
[26]
[27]
[28]
[29]
[30]
[31]

{"sheet":"Sheet1","index":18,"n_rows":24,"n_cols":6,"rows_kept":24,"cut":false,"hidden":true,"merged":[]}
[]
[null,"ID","E",null,"Date Recorded",1]
[null,"UNIQUE ID","F",null,"Type of Deficiency",2]
[1,"Date Recorded","G",null,"Observer code",3]
["ignore","Vessel Type","H",null,"Type of Inspection",4]
[null,"Internal / External","I",null,"Description of Deficiency",5]
[null,"Drydock","J",null,"Equipment Categories",6]
[null,"Information Sharing","K",null,"Area of Observation",7]
[null,"Critical_item","L",null,"Deficiency Cause",8]
[null,"Deficiency Type","M",null,"VIQ Ref Number",9]
[null,"Deficiency Cause","N",null,"Risk Value of Obs",10]
[null,"Inspection Type","O",null,"PSC Ref Number",11]
[null,"Equipments","P",null,"PSC MOU ID",12]
[null,"VIQ Reference Number","Q",null,"Action Taken or Required",13]
[null,"Risk Value of the observation","R",null,"Target Date",14]
[null,"PSC Reference Number","S",null,"PO Ref No.",15]
[null,"PSC MOU","T",null,"Status Code",16]
[null,"Observer Code","U",null,"Date Completed",17]
[null,"Target Date","V",null,"Drydock",18]
[null,"Status Code","W",null,"Info Sharing",19]
[null,"Description of Deficiency","X",null,"Critical Item Flag",20]
[null,"Action taken / required","Y",null,"Audit Type",21]
[null,"PO ref no","Z"]
[null,"Date completed","AA"]

{"sheet":"Ship_information","index":19,"n_rows":2,"n_cols":3,"rows_kept":2,"cut":false,"hidden":true,"merged":[]}
["Ship_ID","Ship_Name","FILE_NAME"]
["23","DHT HAWK (02-12-2021)","23_1638432777991.xlsm"]

{"sheet":"External_Deficiency_type","index":20,"n_rows":5,"n_cols":3,"rows_kept":5,"cut":false,"hidden":true,"merged":[]}
["TITLE","Type of deficiency_description","ID"]
["Condn of Class / Memo",null,5]
["Defect",null,1]
["Non Conformity",null,2]
["Observation",null,3]

{"sheet":"External_Inspection_type","index":21,"n_rows":11,"n_cols":2,"rows_kept":11,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Cargo Audit",17]
["Flag State Insp.",5]
["ISM Audit",2]
["ISPS Audit",3]
["MLC Audit",1]
["Nav Audit / Verification",8]
["OM Insp. (Eg. SIRE / CDI etc.)",6]
["Others (Eg. Insurance etc.)",12]
["PSC Inspection",4]
["Terminal Insp.",11]

{"sheet":"External_Observer_code","index":22,"n_rows":7,"n_cols":3,"rows_kept":7,"cut":false,"hidden":true,"merged":[]}
["TITLE","Observer_code_description","ID"]
["Class Surveyor",null,4]
["FSC Inspector",null,5]
["Others (Eg. Insurance etc.)",null,9]
["PSC Insp.",null,6]
["SIRE / CDI Insp.",null,8]
["Terminal Insp.",null,7]

{"sheet":"Sheet Version","index":23,"n_rows":2,"n_cols":2,"rows_kept":2,"cut":false,"hidden":true,"merged":[]}
["Version","Title"]
["2.0","Version 2.0"]