{"text_format":"1","workbook":"xlsx","n_sheets":24,"sheets":["Mainsheet","Completed","Calc","Areaofobs","Vessel_type","Deficiency_type","VIQrefno","Equipment_list","PSC_MOU","Inspection_type","Deficiency_Cause","Observer_code","Status_code","PSC_ref_no","Risk_value_of_obs","Year","Month","Date_","Sheet1","Ship_information","External_Deficiency_type","External_Inspection_type","External_Observer_code","Sheet Version"],"not_rendered":{"charts":0,"images":5,"macros":1,"external_links":0,"defined_names":12,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Mainsheet","index":0,"n_rows":67,"n_cols":28,"rows_kept":67,"cut":false,"hidden":false,"merged":[[10,8,10,9],[10,12,10,13],[12,6,12,27],[8,6,8,27]]}
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,"Defect - Damage Monitoring Sheet"]
[]
[null,null,null,null,null,null,null,"Date of Report","10-Mar-2022",null,null,"Ship Name","AQUARIUS (10-03-2022)"]
[]
[null,null,null,null,null,null,"VERSION : 2.0"]
[]
[]
[]
[null,null,null,null,"ID","UNIQUE ID","Date Recorded","Type of Deficiency","Observer code","Type of Inspection","Description of Deficiency","Equipment Categories","Area of Observation","Deficiency Cause","VIQ Ref Number","Risk Value of Obs","PSC Ref Number","PSC MOU ID","Action Taken or Required","Target Date","PO Ref No.","Status Code","Date Completed","Drydock","Info Sharing","Critical Item","Audit Type","Superintendent Remarks"]
[null,null,null,null,23351,"26_4 Jan 2022 9:23:08 AM","2021-01-31","Defect","Ship Staff","Ship Staff Insp.","During maintenance on steam line observed some place supporting angle bar corroded and hole in some place on steam line.","Deck - Pipe / Fittings","General Appearance","Equipment Related","","","","","All corroded angle bar need to cut and renew,some steam pipe need to change.","2022-05-31","","Deferred to D D",null,"Yes","No","No","Internal","DD spec to be made"]
[null,null,null,null,19036,"26_30 Apr 2021 8:43:05 AM","2021-04-28","Defect","Ship Staff","Ship Staff Insp.","Cargo Tank Dipping rod tape is in Broken condition","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.12","Medium","","","Vessel will raise an RO for the Tape, Dipping rod and handle of Dipping rod on urgent basis.","2022-05-31","AQUA210070","Waiting spare",null,"No","No","No","Internal","FOR CPP CARGOES, DIPPING ROD IS NOT ALLOWED TO USE FOR GAUGING."]
[null,null,null,null,23352,"26_25 Dec 2021 5:10:41 PM","2021-07-22","Defect","Ship Staff","Ship Staff Insp.","Immersion suit box in forwrd is in wasted condition.","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","Full new box need to be fabricated and shauld be fixed in fwd.","2022-05-31","","Deferred to D D",null,"Yes","No","No","Internal","material on board to fabricate"]
[null,null,null,null,22621,"26_5 Sep 2021 11:03:34","2021-08-25","Defect","Ship Staff","Ship Staff Insp.","Stbd water ballast p/p was not able to start, priming mode in auto.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","Checked found evacuation system float switch defective same need to renew. Requisition raised. Spares received will carry out this job in DD.","2022-03-28","AQUA210131","In progress",null,"Yes","No","No","Internal","Spares supplied."]
[null,null,null,null,16324,"26_30 Dec 2020 1:39:54 PM","2021-08-31","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Weather tight door for Hospita retention bar wasted.","Accommodation","Structural Condn. / WT integrity ","External Factors","","","","","Wasted material(Retention bar) to renew and then paint door portion.","2022-05-31","","In progress",null,"No","No","No","Internal","renew wasted area material and apply  protection"]
[null,null,null,null,22622,"26_4 Oct 2021 10:36:17","2021-09-03","Defect","Ship Staff","Ship Staff Insp.","COT no#1 (P), 2 (P & S), 4 (P & S), 5 (P & S) high level alarm didn’t occurred, after loading the cargo more than 95%.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","After discharging 2 (P & S) both sensors removed and found high level float has lost its buoyancy. both repalced with spare floats. Now COT no#2 P and S high level alarm is working as per order. For No#1 (P), 4 W and 5W, new floats required. Requisition raised for the floats. Float received and all the tanks defective float replaced. Job will be closed after the loading operational check.","2022-05-31","AQUA210138","In progress",null,"No","No","No","Internal","RO supplied at yesou. Carry out spare replacement."]
[null,null,null,null,22625,"26_1 Nov 2021 10:46:43","2021-10-15","Defect","Ship Staff","Ship Staff Insp.","Galley air con is not working.","Accommodation","General Appearance","Equipment Related","","","","","Circuit checked found temperature controller defective. Need to replace. Requisition raised for the same.","2022-05-31","AQUA220012","Waiting spare",null,"No","No","No","Internal","Spares will be connected at Singapore / Korea call."]
[null,null,null,null,22627,"26_17 Nov 2021 6:45:36 PM","2021-10-20","Defect","Ship Staff","Ship Staff Insp.","Slop wings P/V valve supprt stay wire found wasted during inspection.","Deck - Pipe / Fittings","General Appearance","Equipment Related","","","","","Slop wings P/V valve supprt stay wire needs to be renewed.","2022-05-31","","In progress",null,"No","No","No","Internal","Vessel has wires onboard to renew"]
[null,null,null,null,22540,"26_Wed Nov 10 2021 11:27:57 GMT+0000","2021-10-22","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Steam Observation tank side glass to fix","Deck - Machinery","Cargo / Ballast Systems","Equipment Related","","","","","Glass opaque and leaking","2022-05-31","","In progress",null,"No","No","No","Internal","renew glass with spare"]
[null,null,null,null,22541,"26_Wed Nov 10 2021 11:28:42 GMT+0000","2021-10-22","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Mooring winch coupling allen bolt found broken","Deck - Mooring Machinery","Mooring","Equipment Related","","","","","Allen bolts to be renewed and others to be checked","2022-05-31","","In progress",null,"No","No","No","Internal","Check and rewed Allen bolts"]
[null,null,null,null,22542,"26_Wed Nov 10 2021 11:29:43 GMT+0000","2021-10-22","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Void Space 6P and 6S\nManhole rubber Packing to renew","Hull & Tanks","Structural Condn. / WT integrity ","Equipment Related","","","","","Packing to  be renewed","2022-02-28","","In progress",null,"No","No","No","Internal","Check other manhole packing status."]
[null,null,null,null,22543,"26_Wed Nov 10 2021 11:30:50 GMT+0000","2021-10-22","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","No:2 Manifold Valve - Port Side Broken wheel of the manifold valve to repair.","Cargo Mach.,Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","","","","","wheel to be renewed","2022-02-28","","In progress",null,"No","No","No","Internal","Check other valve  wheel condition"]
[null,null,null,null,22544,"26_Wed Nov 10 2021 11:31:36 GMT+0000","2021-10-22","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Forecastle Bilge Valve noted in stuck position, to renew","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","","","","","valve to be renewed","2022-02-28","","In progress",null,"No","No","No","Internal","send order if valve in bad condition"]
[null,null,null,null,22545,"26_Wed Nov 10 2021 11:32:38 GMT+0000","2021-10-22","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Foam Monitor - Port Side Accomodation valve to ease up","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","ease up valve","2022-02-28","","In progress",null,"No","No","No","Internal","regular greasing of monitors to be done"]
[null,null,null,null,22548,"26_Wed Nov 10 2021 11:36:47 GMT+0000","2021-10-22","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Main Deck - Fire line found Corroded section to renew","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","derust line and check and renew thinned down pipe","2022-02-28","","In progress",null,"No","No","No","Internal","vessel has material to renew"]
[null,null,null,null,22549,"26_Wed Nov 10 2021 11:38:30 GMT+0000","2021-10-22","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","WBT (NO2 WBT Stbd side) Tank Dome Cover Hinges found broken, to repair","Hull & Tanks","Cargo / Ballast Systems","Equipment Related","","","","","Hinge to renew after dismantling","2022-02-28","","In progress",null,"No","No","No","Internal","Check all other tank dome hinges"]
[null,null,null,null,22552,"26_Wed Nov 10 2021 11:43:10 GMT+0000","2021-10-22","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","After peak tank vent cover found corroded.","Hull & Tanks","Cargo / Ballast Systems","Equipment Related","","","","","Vent cover  to be repaired","2022-02-28","","In progress",null,"No","No","No","Internal","Check all other air vents"]
[null,null,null,null,22554,"26_Wed Nov 10 2021 11:44:47 GMT+0000","2021-10-22","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Deck fresh water pipe found corroded and holed","Deck - Pipe / Fittings","General Appearance","Equipment Related","","","","","pipe lines to be renewed","2022-02-28","","In progress",null,"No","No","No","Internal","renew partially and others line  renew during  DD"]
[null,null,null,null,22558,"26_Wed Nov 10 2021 11:53:12 GMT+0000","2021-10-22","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Fresh water Pipe Pin hole leak noted on deck","Deck - Pipe / Fittings","General Appearance","Equipment Related","","","","","renew pipe lines","2022-02-28","","In progress",null,"No","No","No","Internal","renew during voyage others to renew during DD"]
[null,null,null,null,22560,"26_Wed Nov 10 2021 11:58:01 GMT+0000","2021-10-22","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Main Deck- Steam Line Valve extended handle to fabricate and fix","Deck - Pipe / Fittings","General Appearance","Equipment Related","","","","","repair to be done","2022-02-28","","In progress",null,"No","No","No","Internal","check other valve condition"]
[null,null,null,null,22628,"26_13 Nov 2021 1:31:28 PM","2021-10-22","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Main deck - Derusting and painting of flanges and U-bolts required.","Miscellaneous","General Appearance","Equipment Related","","","","","Main deck - Derusting and painting of flanges and U-bolts in progress.","2022-02-28","","In progress",null,"No","No","No","Internal","Derusting and painting to be carried out"]
[null,null,null,null,22629,"26_14 Nov 2021 09:36:32","2021-10-22","Observation","Owner / Marine / Tech. Suptd.","Ship Staff Insp.","Accommodation front walkway to chip, buff and paint.","Miscellaneous","General Appearance","Equipment Related","","","","","Accommodation front walkway to chiping, buffing and painting in progress.","2022-02-28","","In progress",null,"No","No","No","Internal","Kindly update on work progress."]
[null,null,null,null,22633,"26_17 Nov 2021 6:40:10 PM","2021-11-05","Defect","Ship Staff","Ship Staff Insp.","Mooring winches( Fwd 2 Pcs & Aft Spring winch 1 pc) Gear engage & disengage handle found corroded.","Deck - Mooring Machinery","General Appearance","Equipment Related","","","","","Mooring winches( Fwd 2 Pcs & Aft Spring winch 1 pc) Gear engage & disengage handle  to be fabricated and renewed. Work in progress.","2022-05-31","","In progress",null,"No","No","No","Internal","Material onboard and  fabricate."]
[null,null,null,null,22632,"26_17 Nov 2021 5:49:18 PM","2021-11-07","Defect","Ship Staff","Ship Staff Insp.","Deck air pipe near Stbd side manifold found corroded & holed.","Deck - Pipe / Fittings","General Appearance","Equipment Related","","","","","Air pipe need to be fabricated & renewed. Work in progress.","2022-05-31","","In progress",null,"Yes","No","No","Internal","repair to be done and remaining to be completed in DD"]
[null,null,null,null,23353,"26_30 Nov 2021 7:25:55 PM","2021-11-08","Defect","Ship Staff","Ship Staff Insp.","ECDIS KEYBOARD AND MOUSE NOT WORKING","Navigation - ECDIS","Navigation","Equipment Related","","","","","INFORMED TO OFFICE,  SPARES/ TECHNICIAN REQUIRED","2022-05-31","","In progress",null,"No","No","No","Internal","order to be raised and replace at  convenient port."]
[null,null,null,null,23355,"26_3 Jan 2022 2:30:45 PM","2021-12-25","Defect","Ship Staff","Ship Staff Insp.","Port and Stbd Windlass break lining drum observed pitting on the surface.","Deck - Mooring Machinery","Mooring","Equipment Related","","","","","Job should be carried out in Dry Dock","2022-05-31","","Deferred to D D",null,"Yes","No","No","Internal","DD spec to be made"]
[null,null,null,null,24049,"26_16 Jan 2022 18:13:03","2022-01-10","Breakdown","Ship Staff","Ship Staff Insp.","01no. UTI display was showing “No message”. And it become non operational.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","Checked found temp sensor with ullage tape faulty same need to replace. Informed office regarding this issue.","2022-05-31","","In progress",null,"No","No","No","Internal","shore service being arranged"]
[null,null,null,null,24187,"26_9 Mar 2022 2:11:11 PM","2022-03-03","Critical Equipment","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Control Block fo No r2 Steering pump leaking","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","To be attnded during DD","2022-05-31","","Deferred to D D",null,"Yes","No","No","Internal"]
[null,null,null,null,24188,"26_9 Mar 2022 2:12:45 PM","2022-03-05","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","AE Crankcase door relief valve leaking","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","To be attended during DD","2022-05-31","","Deferred to D D",null,"Yes","No","No","Internal"]
[null,null,null,null,24189,"26_9 Mar 2022 2:14:31 PM","2022-03-05","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Air condition control panel display screen defective, cannot acces parameters","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","To be attended during DD","2022-05-31","","Deferred to D D",null,"Yes","No","No","Internal"]
[null,null,null,null,24190,"26_9 Mar 2022 2:16:15 PM","2022-03-05","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Emergnecy Fire pump discharge valve and discharge side reducer to renew, drain line and valve to replace, primimng unit to overhaul","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","","","","","To be attended during DD","2022-05-31","","Deferred to D D",null,"No","No","No","Internal"]
[null,null,null,null,24191,"26_9 Mar 2022 2:18:00 PM","2022-03-05","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","IGG inspection cover covered with sealant","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","To be attended during DD","2022-05-31","","Deferred to D D",null,"Yes","No","No","Internal"]
[null,null,null,null,24192,"26_9 Mar 2022 2:20:25 PM","2022-03-05","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Chemical soot blow line covered with putyy, line to renew","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","To be taken up by ship staff","2022-05-31","","Not Started",null,"Yes","No","No","Internal"]
[null,null,null,null,24193,"26_9 Mar 2022 2:25:21 PM","2022-03-05","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Vibration noted on top of boiler, Main steam line clamp removed ffrom place","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related",null,null,"Not Applicable","Not Applicable","Main steam line clamp fixed back in position .","2022-05-31",null,"Deferred to D D",null,"No","No","No","Internal"]
[null,null,null,null,24194,"26_9 Mar 2022 2:27:11 PM","2022-03-05","Observation","Ship Staff","Ship Staff Insp.","Control air drier if of less capacity, moisture noticed in the control air line","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","To be attended during DD","2022-05-31","","Deferred to D D",null,"Yes","No","No","Internal"]
[null,null,null,null,24195,"26_9 Mar 2022 2:29:07 PM","2022-03-05","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Deck air coompresor discharge flexible hose temporary repair carried out.\t\t","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","To be attended during DD","2022-05-31","","Deferred to D D",null,"Yes","No","No","Internal"]
[null,null,null,null,24196,"26_9 Mar 2022 2:31:02 PM","2022-03-05","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","From purifer to HFO sser tank valve gland leaking and oil soaked lagging to replace","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","To be attended by vessel staff","2022-05-31","","Not Started",null,"Yes","No","No","Internal"]
[null,null,null,null,24197,"26_9 Mar 2022 2:33:49 PM","2022-03-05","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Viscosity recorder not working\t","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","To be attended during DD","2022-05-31","","Deferred to D D",null,"Yes","No","No","Internal"]
[null,null,null,null,24198,"26_9 Mar 2022 7:30:11 PM","2022-03-05","Defect","Ship Staff","Ship Staff Insp.","COT 3S & 5S noted oil during purging","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","Under observation shall update","2022-05-31","","Not Started",null,"Yes","No","No","Internal"]
[null,null,null,null,24199,"26_9 Mar 2022 7:32:26 PM","2022-03-05","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","All ladders in Ballast tank to replace basis conditio","Hull & Tanks","Cargo / Ballast Systems","Equipment Related","","","","","To be attended during DD","2022-05-31","","Deferred to D D",null,"Yes","No","No","Internal"]
[null,null,null,null,24201,"26_9 Mar 2022 2:21:51 PM","2022-03-05","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Scupper line holed near vent fan 3","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","to be taken up by ship staff","2022-03-31","","Not Started",null,"Yes","No","No","Internal"]
[null,null,null,null,24202,"26_9 Mar 2022 2:23:42 PM","2022-03-05","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","EGE inlet lagging to repair","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","To be attended during DD","2022-05-31","","Deferred to D D",null,"Yes","No","No","Internal"]
[null,null,null,null,24203,"26_9 Mar 2022 7:36:39 PM","2022-03-05","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","All Water Ballast Tanks coating damaged","Hull & Tanks","Cargo / Ballast Systems","Equipment Related","","","","","To be taken up during  DD","2022-05-31","","Deferred to D D",null,"Yes","No","No","Internal"]
[null,null,null,null,24204,"26_9 Mar 2022 7:38:08 PM","2022-03-05","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","4S and few other ballast tanks 1st stringer plated corroded, holed and thinned down","Hull & Tanks","Cargo / Ballast Systems","Equipment Related","","","","","To be Postponed to DD","2022-05-31","","Deferred to D D",null,"Yes","No","No","Internal"]
[null,null,null,null,24205,"26_9 Mar 2022 7:39:44 PM","2022-03-05","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Windlass brke liner noted with pitting marks, to be repaired during DD","Deck - Machinery","Mooring","Equipment Related","","","","","To be Postponed to DD","2022-05-31","","Deferred to D D",null,"Yes","No","No","Internal"]
[null,null,null,null,24206,"26_9 Mar 2022 7:42:03 PM","2022-03-05","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Catkwalk supports rusted and heaily corroded at many places","Miscellaneous","General Appearance","Equipment Related","","","","","To be renewed during DD","2022-05-31","","Deferred to D D",null,"Yes","No","No","Internal"]
[null,null,null,null,24207,"26_9 Mar 2022 7:43:38 PM","2022-03-05","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Deck area to spot derust and painting required","Deck - Pipe / Fittings","General Appearance","Equipment Related","","","","","Painting is in progress","2022-05-31","","In progress",null,"Yes","No","No","Internal"]
[null,null,null,null,null,"26_5 Apr 2022 15:45:17","2022-03-15","Defect","Ship Staff","Ship Staff Insp.","AE2 CYLINER HEADS NEED TO BE OVERHAULED","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related",null,null,"Not Applicable","Not Applicable","PREPARING  SPARE CYLINDER HEADS TO INSTALL IN AE2","2022-04-15",null,"Not Started",null,"No",null,null,"Internal"]
[null,null,null,null,null,"26_5 Apr 2022 15:49:32","2022-03-20","Defect","Ship Staff","Ship Staff Insp.","IG NOT WORKING IN AUTO","Inert Gas","Eng. / Strg. Comp.","Equipment Related",null,null,"Not Applicable","Not Applicable","TROUBLESHOOTING IN PROGRESS","2022-04-30",null,"In progress",null,"No",null,null,"Internal"]
[null,null,null,null,null,"26_5 Apr 2022 15:53:11","2022-03-26","Critical Equipment","Ship Staff","Ship Staff Insp.","EMG GEN NOT STOPPING IN AUTO","Critical Equip.","Emgcy. Systems","Equipment Related",null,null,"Not Applicable","Not Applicable","TROUBLESHOOTING IN PROGRESS","2022-04-15",null,"In progress",null,"No",null,null,"Internal"]

{"sheet":"Completed","index":1,"n_rows":498,"n_cols":28,"rows_kept":498,"cut":false,"hidden":false,"merged":[[10,8,10,9],[10,12,10,13],[12,6,12,27],[8,6,8,27]]}
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,"Defect - Damage Monitoring Sheet"]
[]
[null,null,null,null,null,null,null,"Date of Report","10-Mar-2022",null,null,"Ship Name","AQUARIUS (10-03-2022)"]
[]
[null,null,null,null,null,null,"VERSION : 2.0"]
[]
[]
[]
[null,null,null,null,"ID","UNIQUE ID","Date Recorded","Type of Deficiency","Observer code","Type of Inspection","Description of Deficiency","Equipment Categories","Area of Observation","Deficiency Cause","VIQ Ref Number","Risk Value of Obs","PSC Ref Number","PSC MOU ID","Action Taken or Required","Target Date","PO Ref No.","Status Code","Date Completed","Drydock","Info Sharing","Critical Item","Audit Type","Superintendent Remarks"]
[null,null,null,null,10816,"26_30 Jan 2020 3:27:32 PM",null,"Defect","Ship Staff","Suptd. Insp.","IGG Scrubber Tower  sight glass seal leaking.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Requisition raised for sight glass and gasket to renew","2020-04-30","AQUA200022","Completed",null,"No","No","No","Internal","As per update from vessel, complete glass was removed and fitted back correctly to prevent leakage."]
[null,null,null,null,4158,"26_2019-10-24 04:25:56.999","2018-09-21","Breakdown","Ship Staff","Ship Staff Insp.","Remote control for winches from remote stands are not operating","Deck - Mooring Machinery","Mooring","Equipment Related","","","","","Remote stand not in use and not required.To be removed in dry dock if possible.","2019-07-19","","Completed","2019-10-24","No","No","No","Internal"]
[null,null,null,null,4159,"26_2019-10-24 03:01:35.000","2018-09-21","Defect","Ship Staff","Ship Staff Insp.","No canvas covers for mooring ropes on drums.To be stitiched and put in use.","Deck - Mooring Machinery","General Appearance","Human Error","","","","","Mooring ropes covered with canvas.","2019-06-11","","Completed","2019-10-24","No","No","No","Internal"]
[null,null,null,null,4160,"26_2019-10-24 04:34:46.000","2018-09-27","Non Conformity","Ship Staff","Ship Staff Insp.","Canvas cover for magnetic compass missing.","Navigation - Others","Navigation","Equipment Related","","","","","Canvas cover stitched and covered.","2019-11-06","","Completed","2019-10-24","No","No","No","Internal"]
[null,null,null,null,4168,"26_2019-10-24 05:15:47.999","2018-12-22","Defect","Ship Staff","Ship Staff Insp.","Safety latch for lifting hook missing.","Deck - Pipe / Fittings","Cargo / Ballast Systems","External Factors","","","","","Same rectified and replaced.","2019-11-30","","Completed","2019-10-24","No","No","No","Internal"]
[null,null,null,null,8651,"26_Wed Dec 04 2019 09:10:14 GMT+0000 (Coordinated Universal Time)","2019-01-12","Breakdown","Ship Staff","Ship Staff Insp.","Framo / Mooring Winch System Hydraulic Main High Pressure Pipeline busted ","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","","","","","Both High & Low Pressure pipelines drained into system tank, High Pressure pipeline removed and transfered to E/Room workshop and repaired with dubbler. High Pressure line fitted back in place after repairs Both pipelines filled with Hydraulic oil and system pressure tested.","2019-02-12","","Completed","2019-02-12","No","No","No","Internal"]
[null,null,null,null,8669,"26_Sat Dec 21 2019 09:49:29 GMT+0000 (Coordinated Universal Time)","2019-01-18","Defect","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","One synthetic Mooring ropes used as an aft spring had broken strands at lengths,","Miscellaneous","Mooring","Inappropriate Procedure","9.17","High","","","Mooring Ropes renewed with spares available onboard. ","2019-01-18","","Completed","2019-01-20","No","No","No","External"]
[null,null,null,null,8670,"26_Sat Dec 21 2019 10:00:33 GMT+0000 (Coordinated Universal Time)","2019-01-18","Defect","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","Printer to Engine room Alarm monitoring system was out of order. ","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","New printer already recieved onboard which had a wrong typr of connector. Same ordered and rectified prior departing the port. ","2019-02-22","","Completed","2019-01-19","No","No","No","External"]
[null,null,null,null,8671,"26_Sat Dec 21 2019 10:04:56 GMT+0000 (Coordinated Universal Time)","2019-01-18","Defect","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","Fresh water was observed leaking through a hole. IWO slop port tank.","Deck - Machinery","Structural Condn. / WT integrity ","Equipment Related","11.4","Very High","","","Leaking section of FW Pipe overhauled & drction renewed leak stopped. ","2019-02-18","","Completed","2019-01-21","No","No","No","External"]
[null,null,null,null,8672,"26_Sat Dec 21 2019 10:08:27 GMT+0000 (Coordinated Universal Time)","2019-01-18","Defect","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","Two Flood lights ( one on port Bridge wing & other on midship post were found out of order.","Elect. Mach. & Equip.","General Appearance","Equipment Related","11.9","Low","","","Rectified during the inspection.","2019-01-19","","Completed","2019-01-18","No","No","No","External"]
[null,null,null,null,10821,"26_30 Jan 2020 7:12:54 AM","2019-02-02","Observation","FSC Inspector","PSC Inspection","Chemical dosing pump of sewage treatment plant not give out discharge","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","6.14","High","Pollution Prevention","","Chemical dosing pump overhauled and all connection and pipe removed and cleaned.Pump tried out working satisfactory","2019-02-15","","Completed","2019-02-02","No","No","No","External"]
[null,null,null,null,8673,"26_Sat Dec 21 2019 11:47:28 GMT+0000 (Coordinated Universal Time)","2019-02-02","Defect","PSC Insp.","PSC Inspection","No identification check was carried out when PSCO boarded the vessel.","Miscellaneous","ISPS Related","Human Error","","","ISPS","","Crew was trained and strict security implementation completed prior the inspector left the vessel.","2019-02-25","","Completed","2019-11-02","No","No","No","External"]
[null,null,null,null,8674,"26_Sat Dec 21 2019 11:52:30 GMT+0000 (Coordinated Universal Time)","2019-02-02","Defect","FSC Inspector","PSC Inspection","RPM meter of Main Engine on Local manoevvuring platform was showing around 10 rpm ahead when M/E was stopped.","E/R - Main Engine","Emgcy. Systems","Equipment Related","","","Propulsion and auxiliary machinery","","Rectified before the ispector left the vessel. ","2019-02-28","","Completed","2019-02-14","No","No","No","External"]
[null,null,null,null,8675,"26_Sat Dec 21 2019 11:56:01 GMT+0000 (Coordinated Universal Time)","2019-02-02","Defect","PSC Insp.","PSC Inspection","Spoiled food was found in vegetable room","Miscellaneous","General Appearance","Human Error","","","Propulsion and auxiliary machinery","","Same shifted quickly nto garbage area and vegetable room cleaned","2019-02-27","","Completed","2019-11-02","No","No","No","External"]
[null,null,null,null,8652,"26_Fri Dec 20 2019 14:22:18 GMT+0000 (Coordinated Universal Time)","2019-03-12","Breakdown","Ship Staff","Ship Staff Insp.","Leak on 5P cargo pipeline in a place where stripping line of 5P Framo Pump connects to 5P Main Cargo line.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","","","","","Cold work carried out with devcon and corddo bond","2019-06-12","","Completed","2019-12-05","No","No","No","Internal"]
[null,null,null,null,4166,"26_2019-10-24 19:33:00.000","2019-05-08","Defect","Ship Staff","Ship Staff Insp.","Air cooler cleaning line from pump to nozzles and drain back chocked","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Pipe removed and nozzzle cleaned","2019-09-30","","Completed","2019-09-19","No","No","No","Internal"]
[null,null,null,null,4144,"26_2019-10-24 08:32:28.000","2019-05-09","Defect","Ship Staff","Ship Staff Insp.","Scupper no.A2 damaged","Miscellaneous","Structural Condn. / WT integrity ","Equipment Related","","","","","Scupper replaced","2019-06-11","AQUA190245","Completed","2020-01-03","No","No","No","Internal","to be arranged at Singapore call."]
[null,null,null,null,8653,"26_Fri Dec 20 2019 14:33:11 GMT+0000 (Coordinated Universal Time)","2019-05-12","Breakdown","Ship Staff","Ship Staff Insp.","Main Deck air Line leaking at 6 W COT","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","","","","","Deck air line isolated, line removed and transferrd to E/Room for Hot work and fitted back after carrying out hort work","2019-07-12","","Completed","2019-12-07","No","No","No","Internal"]
[null,null,null,null,8668,"26_Sat Dec 21 2019 09:43:48 GMT+0000 (Coordinated Universal Time)","2019-05-21","Defect","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","Records of Engine Room (Part I) ORBs were only available since 02 OCT 2019. Records of earlier ORB part I entries ( for last 3 years required by marpol Annex1, Chapter 3C - Reg 17) were not available.","Miscellaneous","Cert. & Docu.","Industry Issue","2.1","Very High","","","Master advised that the ORB's for that period was not retained & handed over by the last operator. After taken over all ORB's were maintained & retained onboard.","2019-06-21","","Completed","2019-05-22","No","No","No","External"]
[null,null,null,null,8660,"26_Sat Dec 21 2019 07:40:38 GMT+0000 (Coordinated Universal Time)","2019-06-06","Defect","Others (Eg. Insurance etc.)","Others (Eg. Insurance etc.)","Second Engineer national certificate of competency was Marine Engineer Oficer Class II, however as per liberian Flag endorsement for his national COC.he was allowed to serve in capacity of Chief Engineer.","Miscellaneous","Cert. & Docu.","Industry Issue","4.3","Medium","","","Flag state informed & his Liberian endorsement was corrected. ","2019-06-07","","Completed","2019-07-06","No","No","No","External"]
[null,null,null,null,8661,"26_Sat Dec 21 2019 07:58:17 GMT+0000 (Coordinated Universal Time)","2019-06-06","Defect","Others (Eg. Insurance etc.)","Others (Eg. Insurance etc.)","On Wharf ladder which was in use, the load tested to,maximum angle of inclination and date of load test was not marked.","Deck - Machinery","MLC Related","Human Error","","","","","All markings such as load tested/max inclination angle were stencilled on the wharf ladder platform.","2019-07-07","","Completed","2019-06-07","No","No","No","External"]
[null,null,null,null,8662,"26_Sat Dec 21 2019 08:06:48 GMT+0000 (Coordinated Universal Time)","2019-06-06","Defect","Others (Eg. Insurance etc.)","Others (Eg. Insurance etc.)","Engine room 1st deck fire zone was noted isolated and disabled.","Elect. Mach. & Equip.","Emgcy. Systems","Inappropriate Procedure","5.35","Medium","","","Immediately rectificed the zone enabled. And log started when this gets isolated for Hot work in E/Rm workshop.","2019-07-06","","Completed","2019-06-07","No","No","No","External"]
[null,null,null,null,8663,"26_Sat Dec 21 2019 08:10:01 GMT+0000 (Coordinated Universal Time)","2019-06-06","Defect","Others (Eg. Insurance etc.)","Others (Eg. Insurance etc.)","In emergency generator room on 220V emergency switchboard ow isulation of 0.0 Megaohm was noted.","Elect. Mach. & Equip.","Emgcy. Systems","Equipment Related","","","","","Same check & corrected","2019-07-07","","Completed","2019-06-07","No","No","No","External"]
[null,null,null,null,8664,"26_Sat Dec 21 2019 07:50:04 GMT+0000 (Coordinated Universal Time)","2019-06-06","Defect","Others (Eg. Insurance etc.)","Others (Eg. Insurance etc.)","The Carbon Monoxide (CO) low level alarm setting on portable multi gas meters was set at 30 PPM whereas the TLV TWA of CO was 25 PPM. ","Miscellaneous","Cargo / Ballast Systems","Equipment Related","","","","","Correction made on personal gas meters as required druing the next shore servicing. ","2019-06-07","","Completed","2019-07-06","No","No","No","External"]
[null,null,null,null,8665,"26_Sat Dec 21 2019 08:17:22 GMT+0000 (Coordinated Universal Time)","2019-06-06","Other","Others (Eg. Insurance etc.)","Others (Eg. Insurance etc.)","Vessel had cargo hose fro portable framo pump of size 30 m x 8\" x1 no. which was last tested to 5.0 bar on 27-dec-2-18 howerver elongation test & electrical contimnuity test was not carried out and no record was available.","Miscellaneous","Cargo / Ballast Systems","Inappropriate Procedure","","","","","Electirical continuity & elongation test completed & entries made accordingly. ","2019-07-07","","Completed","2019-06-15","No","No","No","External"]
[null,null,null,null,8666,"26_Sat Dec 21 2019 08:24:39 GMT+0000 (Coordinated Universal Time)","2019-06-06","Defect","Others (Eg. Insurance etc.)","Others (Eg. Insurance etc.)","1.Soft patch was noted on steam branch heating line(size 150mm) located on main deck midship area and straub coupling was put to arrest leak. 2. At various places on main deck rust sposts on pipe work","Miscellaneous","General Appearance","Equipment Related","","","","","Steam line renewed with spare pipe available. And continous fabric maintenance upgrade is in progress. ","2019-07-07","","Completed","2019-07-07","No","No","No","External"]
[null,null,null,null,4167,"26_2019-10-24 08:00:46.000","2019-07-18","Defect","Ship Staff","Ship Staff Insp.","Manifold valve port an stbd including the reducer 14''x16'' require dersuting and attention.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","","","","","Dersuting/painting completed.","2019-06-11","","Completed","2019-10-25","No","No","No","Internal"]
[null,null,null,null,4161,"26_2019-10-24 08:18:49.000","2019-07-22","Defect","Ship Staff","Ship Staff Insp.","Main and branches of steam line  inlet and return leaking and corroded at places.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","","","","","All necessary repairs/replacement/painting of all Cargo tank steam lines completed.","2019-11-30","","Completed","2019-10-23","No","No","No","Internal"]
[null,null,null,null,16682,"26_5 Jan 2021 1:00:28 PM","2019-08-04","Observation","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","Communitor not added to Garbage Manangement certificate","Documentation","Cert. & Docu.","Inappropriate Procedure","2.1","Very High","","","Necessay changes made in the certificate by class , same updated and forwarded to vessel.","2019-08-29","","Completed","2019-08-04","No","No","No","External"]
[null,null,null,null,16683,"26_5 Jan 2021 1:05:14 PM","2019-08-04","Observation","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","Entry for ODME when operaional was logged in ORB","Miscellaneous","MARPOL Related","Human Error","6.13","Low","","","Immediately necessary changes as per procedures were made in ORB.","2019-08-19","","Completed","2019-08-04","No","No","No","External"]
[null,null,null,null,8658,"26_Sat Dec 21 2019 07:12:21 GMT+0000 (Coordinated Universal Time)","2019-08-04","Defect","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","The item garbage treatment plant in the certificate of the satement compliance with the equipments for the prevention of pollution by garbage was not selected. Actually one communitor in galley was used.","Miscellaneous","Cert. & Docu.","Industry Issue","2.1","Very High","","","Statement of compliance new issued by class BV","2019-09-04","","Completed","2019-07-08","No","No","No","External"]
[null,null,null,null,8659,"26_Sat Dec 21 2019 07:26:36 GMT+0000 (Coordinated Universal Time)","2019-08-04","Defect","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","Onreview of Oil record book Part II, ODME was fault in measure cell on 21 July 2019, and the system has been made operational on 23 july 2019, but the time of this system operational was not recorded in Oil Record Book again. ","Cargo Mach.","Cargo / Ballast Systems","Human Error","6.13","Low","","","Relevant entries made in the ORB Part II. ","2019-04-09","","Completed","2019-08-05","No","No","No","External"]
[null,null,null,null,8734,"26_Sun Dec 22 2019 14:11:30 GMT+0000 (Coordinated Universal Time)","2019-08-05","Defect","Owner / Marine / Tech. Suptd.","Nav Audit / Verification","No ECDIS repeater panel in Masters cabin","Navigation - ECDIS","Navigation","Equipment Related","","","","","ECDIS Repeater to be fitted in masters cabin","2019-07-06","","Completed","2019-06-05","No","No","No","Internal"]
[null,null,null,null,8735,"26_Sun Dec 22 2019 14:19:22 GMT+0000 (Coordinated Universal Time)","2019-08-05","Defect","Owner / Marine / Tech. Suptd.","Nav Audit / Verification","Magnetic compass deviation more than 15 deg in some heading. ","Navigation - Others","Navigation","Equipment Related","","","","","Magnetic deviation card by shore compass adjustor ","2019-06-30","","Completed","2019-06-20","No","No","No","Internal"]
[null,null,null,null,4163,"26_2019-10-25 11:01:06.000","2019-08-30","Defect","Ship Staff","Ship Staff Insp.","No fresh water supply on deck.Fresh water main line leaking /block and corroded near 1W,3W,5W,6W COT area.","Miscellaneous","Cargo / Ballast Systems","Equipment Related","","","","","All fresh water lines opened /repaired/fabricated & painted.Fresh water supply reinsted right upto forecastle.","2019-10-30","","Completed","2019-10-23","No","No","No","Internal"]
[null,null,null,null,4149,"26_2019-10-24 19:42:09.000","2019-08-31","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Air conditioning compressor drier not replaced since take over.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Air condition plant performance checked found good, No sign of moisture found in system.Requistion raised to maintain ROB onboard.","2020-03-30","AQUA190255","Completed","2020-01-25","No","No","No","Internal","noted"]
[null,null,null,null,4150,"26_2019-10-24 19:44:22.000","2019-08-31","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Provision plant drier not been replaced since take over.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Ref. plant performance checked found satisfactory, No visiual sign of moisture found in system.Requistion raised to maintain ROB onboard. ","2020-03-30","AQUA190256","Completed","2020-01-27","No","No","No","Internal","noted."]
[null,null,null,null,4151,"26_2019-10-24 19:47:10.000","2019-08-31","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ECR telegraph misalignment alarm active.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.33","High","","","Telegraph chain worn out an needs replacement. Requistion raised .","2019-11-30","AQUA190218","Completed","2019-12-05","No","No","No","Internal"]
[null,null,null,null,4152,"26_2019-10-24 19:49:44.000","2019-08-31","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Port side grey water line has minor leak\t","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","OB valve to be renewed with the spare received at Singapore. Awaitng suitable opportunity for vessel in Ballast.","2019-11-30","","Completed","2020-01-15","No","No","No","Internal","noted."]
[null,null,null,null,4153,"26_2019-10-24 19:52:46.000","2019-08-31","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Pressure regulating valve for ME FO line leaking","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Will be renewed in DD while system in MGO","2020-04-30","AQUA190234","Completed","2020-04-30","No","No","No","Internal","Job completion noted."]
[null,null,null,null,4169,"26_2019-10-24 19:38:43.000","2019-08-31","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","No record of steering gear filter replaced since take over","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Filter replaced and record for same maintained near the steering gear.","2019-09-30","","Completed","2019-09-20","No","No","No","Internal"]
[null,null,null,null,4156,"26_2019-10-25 10:52:12.000","2019-09-05","Defect","Ship Staff","Ship Staff Insp.","Port & stbd manifold wheel valves badly corooded.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","","","","","Manifold Valve Wheels replaced","2019-11-30","AQUA190245","Completed","2019-11-04","No","No","No","Internal","Arranging supply at Singapore call."]
[null,null,null,null,8644,"26_Thu Oct 24 2019 08:32:28 GMT+0000 (Coordinated Universal Time)","2019-09-05","Defect","Ship Staff","Ship Staff Insp.","Scupper no.A2 damaged","Miscellaneous","Structural Condn. / WT integrity ","Equipment Related","","","","","Replaced with New Scupper","2019-11-06","AQUA190245","Completed","2019-10-11","No","No","No","Internal"]
[null,null,null,null,8736,"26_Sun Dec 22 2019 14:45:23 GMT+0000 (Coordinated Universal Time)","2019-09-08","Defect","Owner / Marine / Tech. Suptd.","Nav Audit / Verification","DGPS antenna securing arrangement needs maintenance, Vibration at High RPM coupled with strong winds have toppled the antenna.","Navigation - DGPS / EPFS / AIS","Navigation","Equipment Related","","","","","Antenna resecured in place properly","2019-11-11","","Completed","2019-08-10","No","No","No","Internal"]
[null,null,null,null,8655,"26_Fri Dec 20 2019 14:39:46 GMT+0000 (Coordinated Universal Time)","2019-09-12","Defect","Ship Staff","Ship Staff Insp.","Starboard Windlass Hydraulic Pipeline section badly corroded.","Deck - Mooring Machinery","Mooring","Equipment Related","","","","","New Pipeline fabricated and replaced the fabricated section.","2019-12-12","","Completed","2019-12-11","No","No","No","Internal","noted"]
[null,null,null,null,4145,"26_2019-10-24 08:36:33.000","2019-09-17","Defect","Ship Staff","Ship Staff Insp.","Fwd mooring winches hydraulic line connectors for inlet line leaking.","Deck - Mooring Machinery","Mooring","Equipment Related","","","","","Fittings replaced","2019-11-11","","Completed","2019-12-28","No","No","No","Internal","Fittings supplied."]
[null,null,null,null,8645,"26_Thu Oct 24 2019 08:47:52 GMT+0000 (Coordinated Universal Time)","2019-10-02","Defect","Ship Staff","Ship Staff Insp.","2 Fresh water valve  near 2W & 3W COT area found leaking.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","","","","","Replaced Valves","2019-11-06","AQUA190245","Completed","2019-01-11","No","No","No","Internal","Noted FW valves replaced"]
[null,null,null,null,8738,"26_Sun Dec 22 2019 14:55:11 GMT+0000 (Coordinated Universal Time)","2019-10-08","Defect","Owner / Marine / Tech. Suptd.","Mooring Audit","Brake band on Stbd Windlass needs renewal","Deck - Mooring Machinery","Mooring","Equipment Related","","","","","Brake bands renewed ","2019-08-11","","Completed","2019-09-16","No","No","No","Internal"]
[null,null,null,null,8739,"26_Sun Dec 22 2019 15:00:56 GMT+0000 (Coordinated Universal Time)","2019-10-08","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","PV Breaker level gauge transparent cover dirty- same needs to be cleaned/ renewed.","Miscellaneous","Cargo / Ballast Systems","Equipment Related","","","","","Level gauge glass renewed.","2019-08-11","","Completed","2019-09-08","No","No","No","Internal"]
[null,null,null,null,8740,"26_Sun Dec 22 2019 15:04:41 GMT+0000 (Coordinated Universal Time)","2019-10-08","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Ballast water record log book not used for record keeping.REcords filled in printed forms.","Documentation,Miscellaneous","Cargo / Ballast Systems","Inappropriate Procedure","","","","","New record books started & information transfered into log book from forms. ","2019-10-09","","Completed","2019-08-14","No","No","No","Internal","Noted"]
[null,null,null,null,8741,"26_Sun Dec 22 2019 15:19:06 GMT+0000 (Coordinated Universal Time)","2019-10-08","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Manifold reducres needs maintenance & inspection. ","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","","","","","Fabric maintenance completed on all manifold reducres. A few new ones ordered. ","2019-10-11","","Completed","2019-11-09","No","No","No","Internal"]
[null,null,null,null,4164,"26_2019-10-24 20:02:19.000","2019-10-10","Defect","Ship Staff","Ship Staff Insp.","Main Engine fuel valve testing machine FO container cracked","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Acrylic sheet cover created for same.","2019-10-25","","Completed","2019-10-23","No","No","No","Internal","Noted."]
[null,null,null,null,4162,"26_2019-10-24 09:12:04.999","2019-10-24","Defect","Ship Staff","Ship Staff Insp.","Fire line no.2 port side near fwd spring winch found leaking from 2 places due to pin hole.","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","New pipe fabricated and put in place.","2019-10-24","","Completed","2019-10-25","No","No","No","Internal","Noted"]
[null,null,null,null,8646,"26_Fri Nov 15 2019 17:38:00 GMT+0000 (Coordinated Universal Time)","2019-11-01","Defect","Ship Staff","Ship Staff Insp.","VRCS auto start and stop of Pump No 2 not working","Deck - Machinery","Mooring","Equipment Related","","","","","Requiasiton raised","2019-11-20","AQUA 190278","Completed","2019-11-15","No","No","No","Internal","Noted"]
[null,null,null,null,8647,"26_Fri Nov 15 2019 17:44:25 GMT+0000 (Coordinated Universal Time)","2019-11-06","Defect","Ship Staff","Ship Staff Insp.","LT cooler SW inlet pipe leaking","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Pipe renewed","2019-11-20","","Completed","2019-11-12","No","No","No","Internal","Noted"]
[null,null,null,null,8641,"26_Fri Nov 15 2019 08:43:41 GMT+0000 (Coordinated Universal Time)","2019-11-11","Defect","Ship Staff","Ship Staff Insp.","Deck Seak SW Filling line found to be leaking","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","","","","","SW filling pump to be stopped, SW filling line to be removed and new SW filling line to be fabricated.","2019-11-13","","Completed","2019-11-14","No","No","No","Internal"]
[null,null,null,null,8642,"26_Fri Nov 15 2019 09:20:14 GMT+0000 (Coordinated Universal Time)","2019-11-11","Defect","Ship Staff","Ship Staff Insp.","Fire Branch Line on 6w COT found Leaking.","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","Fire Branch line to be removed and transfered to E/Room workshop to carry out Hot Work","2019-11-14","","Completed","2019-11-14","No","No","No","Internal","Noted"]
[null,null,null,null,8638,"26_Fri Nov 15 2019 17:54:08 GMT+0000 (Coordinated Universal Time)","2019-11-12","Defect","Ship Staff","Ship Staff Insp.","AE No 3 LO temperature rising during operation.\t","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","To renew thermostatic valve. Requisition raised.","2019-12-25","AQUA 190247","Completed","2020-01-06","No","No","No","Internal","Will be supplied at coming port call."]
[null,null,null,null,8643,"26_Fri Nov 15 2019 09:35:52 GMT+0000 (Coordinated Universal Time)","2019-11-14","Defect","Ship Staff","Ship Staff Insp.","Fire Branch Line at 2w COT found leaking","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","Fire branch line to be removed and transfered to E/room Workshop to carry out hot work","2019-11-16","","Completed","2019-11-16","No","No","No","Internal","Noted"]
[null,null,null,null,8639,"26_Sat Nov 23 2019 06:33:36 GMT+0000 (Coordinated Universal Time)","2019-11-20","Defect","Ship Staff","Ship Staff Insp.","SOME OF NATURAL VENT FLAPS FOR ACCOMODATION ARE CORRODED AND WASTED.","Accommodation","Structural Condn. / WT integrity ","Equipment Related","","","","","Wasted areas repaired with inserts by taking the vent flaps in E/Room Workshop","2019-12-05","","Completed","2019-12-23","No","No","No","Internal","noted and pls send details so that we can ask ashore for fabrication."]
[null,null,null,null,8648,"26_Sat Nov 23 2019 06:43:54 GMT+0000 (Coordinated Universal Time)","2019-11-21","Breakdown","Ship Staff","Ship Staff Insp.","Steam Line leaking on 2 sections of Main Steam line.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","","","","","Main Steam line Isolated, Main Steam Line removed from place and taken to E/Room, 1 section Fabricated with new Pipeline and other line repaired.","2019-11-22","","Completed","2019-11-22","No","No","No","Internal","Noted"]
[null,null,null,null,4133,"26_2019-10-24 05:07:30.000","2019-11-25","Defect","Ship Staff","Ship Staff Insp.","Pipelines on main deck require cosmetic upgradation","Deck - Pipe / Fittings","General Appearance","Equipment Related","","","","","Dersuting and painting works for main deck pipelines & steam line in progress.","2020-04-26","","Completed","2020-04-15","No","No","No","Internal","This is ongoing job."]
[null,null,null,null,8657,"26_Wed Dec 04 2019 06:34:02 GMT+0000 (Coordinated Universal Time)","2019-11-26","Breakdown","Ship Staff","Ship Staff Insp.","Ballast tank vent covers of 1S, 1P & 2P WBT are corroded and wasted.","Hull & Tanks","Structural Condn. / WT integrity ","Equipment Related","","","","","New covers fabricated and replaced the wasted covers.","2019-06-12","","Completed","2019-06-12","No","No","No","Internal","Noted"]
[null,null,null,null,8737,"26_Sun Dec 22 2019 14:51:32 GMT+0000 (Coordinated Universal Time)","2019-12-08","Defect","Owner / Marine / Tech. Suptd.","Nav Audit / Verification","The Ships Bell required on forward section of the vessel is missing. Required as per Colregs","Navigation - Others","Navigation","Equipment Related","","","","","Ships bell fitted back in place on teh forward mast. ","2019-11-09","","Completed","2019-08-15","No","No","No","Internal"]
[null,null,null,null,8640,"26_Fri Dec 20 2019 16:19:13 GMT+0000 (Coordinated Universal Time)","2019-12-17","Breakdown","Ship Staff","Ship Staff Insp.","Main Steam Line Section at 2W CoT is Leaking","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","","","","","Section removed and taken to E/Room for fabrication of new steam line","2019-12-22","","Completed","2019-12-22","No","No","No","Internal","Noted that pipe section fabricated and completed. Pls check other lines too and report."]
[null,null,null,null,8654,"26_Fri Dec 20 2019 14:54:12 GMT+0000 (Coordinated Universal Time)","2019-12-17","Breakdown","Ship Staff","Ship Staff Insp.","Port Windlass Hydraulic Pipe line leaking","Deck - Mooring Machinery","Mooring","Equipment Related","","","","","Hydraulic PipeLine removed transfered to E/Room carried out hot work and and fitted back","2019-12-19","","Completed","2019-12-18","No","No","No","Internal","Noted. Please completely check all other hydraulic lines closely to ensure the health is good."]
[null,null,null,null,8656,"26_Fri Dec 20 2019 16:13:20 GMT+0000 (Coordinated Universal Time)","2019-12-17","Breakdown","Ship Staff","Ship Staff Insp.","Main Deck Air Pipeline at 5W COT's  Leaking","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","","","","","Deck air isolated, Leaking section of Main deck air pipeline removed, New pipeline fabricated and replaced.","2019-12-20","","Completed","2019-12-19","No","No","No","Internal","Noted. Please check the complete deck air line and rectify any other leaks."]
[null,null,null,null,9729,"26_2020-01-15 3:31:43 PM","2020-01-01","Observation","Ship Staff","Ship Staff Insp.","Slop S Steam Supply branch line found leaking.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","","","","","Slop S Steam Manifold isolated form Main stem line, Defective section removed and transferred to E/Room, hot work carried out and fitted back in place.","2020-01-14","","Completed","2020-01-14","No","No","No","Internal","Noted."]
[null,null,null,null,10820,"26_2020-01-27 3:26:12 AM","2020-01-14","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Mooring Winch Hydraulic Brake hoses to be renewed.","Deck - Mooring Machinery","Mooring","Equipment Related","","","","","Mooring Winch Hydraulic Brake hoses checked and found in good condition. vessel has 1 spare hose.","2020-02-25","","Completed","2020-01-16","No","No","No","Internal"]
[null,null,null,null,10833,"26_2020-01-27 2:02:31 PM","2020-01-14","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","port anchor Bow Stopper pin has thinned down same to be ordered and renewed.","Deck - Mooring Machinery","Mooring","Equipment Related","","","","","New Pin Fabricated","2020-02-24","","Completed","2020-02-18","No","No","No","Internal"]
[null,null,null,null,10812,"26_2020-01-28 4:31:04 AM","2020-01-16","Defect","Ship Staff","Ship Staff Insp.","Mooring Winch Hydraulic Brake cylinder head seal is leaking, Same required to be changed.","Deck - Mooring Machinery","Mooring","Equipment Related","","","","","All Leaking Hydraulic brake cylinder seals changed.","2020-03-25","AQUA200024","Completed","2020-03-25","No","No","No","Internal","Hoses were already supplied and renewed  by staff. As well  as seals were renewed. \nNow few ones, relief valves need replacement., we will supply once requisition is raised. \nManual breaks are in good order."]
[null,null,null,null,10828,"26_2020-01-30 12:05:43 PM","2020-01-21","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Manifold Flanges and Reducers to be De-Rusted and Painted","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","","","","","Manifold Flanges and Reducers  De-Rusted and Painted","2020-01-22","","Completed","2020-01-22","No","No","No","Internal"]
[null,null,null,null,16684,"26_5 Jan 2021 12:33:33 PM","2020-01-22","Observation","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","Launching procedures for liferaft missing","LSA / FFA","Safety / LSA / FFA","External Factors","5.28","Very High","","","two poster for procedures to launch liferaft were ordered same put in place prior departure.","2020-02-07","","Completed","2020-01-23","No","No","No","External"]
[null,null,null,null,16685,"26_5 Jan 2021 12:37:17 PM","2020-01-22","Observation","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","Two bolts on port side bunker manifold were not extending out of the nuts.","Cargo Mach.","Cargo / Ballast Systems","Knowledge Based","8.41","Medium","","","Immediately the bolts were renewed with correct size .","2020-02-07","","Completed","2020-01-22","No","No","No","External"]
[null,null,null,null,16686,"26_5 Jan 2021 12:52:11 PM","2020-01-22","Observation","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","Engineer call alarm activitaed after 5 min","Miscellaneous","Safety / LSA / FFA","Knowledge Based","10.14","Medium","","","Same was reset to 3 min and tested.","2020-02-07","","Completed","2020-01-22","No","No","No","External"]
[null,null,null,null,10810,"26_2020-01-26 7:49:49 AM","2020-01-24","Observation","Ship Staff","Ship Staff Insp.","Grating on Catwalk and PV Valve stands are badly corroded.","Deck - Pipe / Fittings","General Appearance","Equipment Related","","","","","Gratings on Catwalk changed. Changing of gratings on PV Valves Stands and Access to Catwalk in progress","2020-04-15","AQUA200005","Completed","2020-04-15","No","No","No","Internal","NOTED THAT GRATINGS RENEWAL DONE WITH SUPPLIED UNITS."]
[null,null,null,null,10825,"26_30 Jan 2020 3:37:18 PM","2020-01-24","Defect","Ship Staff","Ship Staff Insp.","Deck seal sea water line internal diameter reduced due to scale deposits  ","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Deck seal sea water line to renew from pump to Deck Seal Tank  ","2020-03-01","","Completed","2020-02-04","No","No","No","Internal"]
[null,null,null,null,10819,"26_2020-01-26 7:53:16 AM","2020-01-25","Defect","Ship Staff","Ship Staff Insp.","Aft Spring Mooring winch hydraulic return pipeline found leaking.","Deck - Pipe / Fittings","Mooring","Equipment Related","","","","","New pipeline to be fabricated and replaced the damaged pipeline.","2020-01-28","","Completed","2020-01-28","No","No","No","Internal"]
[null,null,null,null,10831,"26_30 Jan 2020 3:31:37 PM","2020-01-25","Defect","Ship Staff","Ship Staff Insp.","Scrubber cooling sea water inlet pipe from scrubber pump to Tower section thinned down. ","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Pipe renewed","2020-03-04","","Completed","2020-03-10","No","No","No","Internal"]
[null,null,null,null,10813,"26_2020-01-30 11:40:51 AM","2020-01-29","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Main deck area bays - COT 2w, 3w, 4w and under manifold areas has scattered rust on\n\nthe deck, Transverse beams and under pipeline supports.","Deck - Pipe / Fittings","General Appearance","Equipment Related","","","","","Hydro-Blasting to be carried out followed by Buffing / Primer / Painting","2020-04-30","","Completed","2020-04-30","No","No","No","Internal","NOTED VIA WEEKLY WORK DONE REPORT. ENSURE DECK AREAS ARE MAINTAINED RUST FREE ."]
[null,null,null,null,10815,"26_2020-01-30 12:11:38 PM","2020-01-29","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Aft superstructure to be de-rusted and panted. All Primered areas to be final coated. Funnel deck and other accommodation decks to be painted.","Accommodation ","General Appearance","Equipment Related","","","","","Superstructure Aft From Bridge Deck to A-Deck De-Rusted, Buffing Carried out followed by 1st Coat Primer and 2nd Coat Primer. Bridge Deck Full Coat carried out for Bulkhead and Exterior Deck.","2020-04-15","","Completed","2020-04-15","No","No","No","Internal","JOB WELL DONE!"]
[null,null,null,null,10822,"26_2020-01-30 11:45:23 AM","2020-01-29","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Hydro blasting of mooring winches on Forecastle to be completed.","Deck - Mooring Machinery","Mooring","Equipment Related","","","","","Hydro Blasting Followed by Buffing / 1st Coat Primer/ 2nd Coat Primer Carried out. Ful l coat painting carried out.","2020-02-13","","Completed","2020-01-02","No","No","No","Internal"]
[null,null,null,null,10834,"26_2020-01-30 12:01:29 PM","2020-01-29","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Steam Supply Line for 5W COT Required to be fabricated.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","","","","","New Steam Pipeline fabricated and replaced the damged sections.","2020-02-13","","Completed","2020-05-03","No","No","No","Internal"]
[null,null,null,null,10823,"26_9 Feb 2020 7:38:47 AM","2020-02-03","Defect","Ship Staff","Ship Staff Insp.","Main Deck Air pipeline at 5W CoT Leaking.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","","","","","Main Deck air pipeline section removed and replaced with new fabricated pipeline,","2020-02-09","","Completed","2020-02-08","No","No","No","Internal"]
[null,null,null,null,11336,"26_4 Apr 2020 1:11:45 PM","2020-02-03","Breakdown","Ship Staff","Ship Staff Insp.","Boiler water Circulating Pump leaking No.2","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Pump overhauled and put in service","2020-03-29","AQUA205008","Completed","2020-03-28","No","No","No","Internal"]
[null,null,null,null,10824,"26_9 Feb 2020 7:43:38 AM","2020-02-05","Defect","Ship Staff","Ship Staff Insp.","No. 4 Foam Monitor found ceased and not rotating 360 Deg.","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","Foam Monitor overhauled and greased.","2020-02-08","","Completed","2020-02-07","No","No","No","Internal"]
[null,null,null,null,10832,"26_10 Mar 2020 1:42:31 PM","2020-02-08","Breakdown","Ship Staff","Ship Staff Insp.","STP Plant blower motor winding got damaged and giving low insulation.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Motor renewed along with blower","2020-02-29","","Completed","2020-03-02","No","No","No","Internal"]
[null,null,null,null,10826,"26_2020-02-19 11:43:56 AM","2020-02-19","Defect","Ship Staff","Ship Staff Insp.","Hose Handling Crane Jib Head Sheavs found Not moving.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","Sheaves revomed and overhauled and greased.","2020-03-15","","Completed","2020-02-29","No","No","No","Internal"]
[null,null,null,null,10827,"26_2020-02-19 11:47:35 AM","2020-02-19","Defect","Ship Staff","Ship Staff Insp.","Port Side Ballast Pump Deck Air priming line found leaking.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","Pipe sections removed and transfered to Engine room  work shop, new sections fabricated and replaced the damaged sections.","2020-02-21","","Completed","2020-02-21","No","No","No","Internal"]
[null,null,null,null,10829,"26_1 Mar 2020 6:47:05 AM","2020-02-23","Defect","Ship Staff","Ship Staff Insp.","Fwd Steam By-Pass pile line section found leaking","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","","","","","Pipeline section removed and transferred to Engine room workshop, New pipeline fabricated and replaced the damaged section.","2020-02-29","","Completed","2020-02-29","No","No","No","Internal"]
[null,null,null,null,10830,"26_1 Mar 2020 6:49:31 AM","2020-02-23","Defect","Ship Staff","Ship Staff Insp.","3S Steam Manifold Pipeline Section found Leaking.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","","","","","Pipeline section removed and transferred to Engine room workshop, New pipeline fabricated and replaced the damaged section.","2020-02-29","","Completed","2020-02-29","No","No","No","Internal"]
[null,null,null,null,10835,"26_1 Mar 2020 6:52:31 AM","2020-02-24","Defect","Ship Staff","Ship Staff Insp.","4W Steam branch pipeline leaking.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","","","","","4W Steam Branch Pipeline Repaired.","2020-03-03","","Completed","2020-03-03","No","No","No","Internal"]
[null,null,null,null,10811,"26_2020-01-27 3:13:14 AM","2020-02-28","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Temperature Sensor of 2P COT Showing erratic.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","2P COT Temprature sensor Renewed.","2020-05-30","AQUA205006","Completed","2020-05-15","No","No","No","Internal","Spare sensor is ordered  ; PO no. AQUA205006 sensor is now connected on board."]
[null,null,null,null,11337,"26_4 Apr 2020 1:18:05 PM","2020-03-11","Breakdown","Ship Staff","Ship Staff Insp.","Scrubber pump suction line T section leaking,pipe holed","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.31","Very High","","","new pipe fabricated and fixed.","2020-03-14","","Completed","2020-03-19","No","No","No","Internal"]
[null,null,null,null,11332,"26_2020-03-17 8:51:38 AM","2020-03-13","Defect","Ship Staff","Ship Staff Insp.","Sbtd mooring winch Hydraulic pipeline on Poop deck found leaking.","Deck - Mooring Machinery","Mooring","Equipment Related","","","","","New sections fabricated and replaced the old leaking sections.","2020-03-16","","Completed","2020-03-15","No","No","No","Internal"]
[null,null,null,null,11338,"26_2020-03-17 8:34:38 AM","2020-03-13","Defect","Ship Staff","Ship Staff Insp.","3 Sections of Deck Air line for Stbd Ballast pump found  leaking. ","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","","","","","1 Section fabricated and renewed, Fabrication of 2 new sections in progress.","2020-03-20","","Completed","2020-03-20","No","No","No","Internal"]
[null,null,null,null,11331,"26_2020-03-17 8:43:51 AM","2020-03-14","Defect","Ship Staff","Ship Staff Insp.","Deck Air Pipeline for Port and Stbd gangway and badly corroded. ","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","","","","","New Sections fabricated and changed the corroded sections for port and Stbd deck air supply pipeline.","2020-03-15","","Completed","2020-03-15","No","No","No","Internal"]
[null,null,null,null,4136,"26_2019-10-24 05:25:49.999","2020-03-15","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Supports for conduit/pipes to de-rust and paint soon; rust on deck is mainly spreading due to rusty tray","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","","","","","Work in progress","2020-05-15","","Completed","2020-04-15","No","No","No","Internal","THIS IS REGULAR MAINTENANCE JOB AND NEEDS CONTINUOUS MONITORING AND MAINTENANCE."]
[null,null,null,null,11333,"26_2020-03-17 8:57:12 AM","2020-03-15","Defect","Ship Staff","Ship Staff Insp.","Slop Steam Supply pipeline section found leaking.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","","","","","New section fabricated and replaced the leaking section.","2020-03-18","","Completed","2020-03-16","No","No","No","Internal"]
[null,null,null,null,11325,"26_2020-03-17 10:14:53 AM","2020-03-16","Defect","Ship Staff","Ship Staff Insp.","Aft Spring Mooring winch Hydraulic brake relief valve badly corroded and found leaking.","Deck - Mooring Machinery","Mooring","Equipment Related","","","","","Hydraulic Brake control block changed","2020-05-31","","Completed","2020-05-15","No","No","No","Internal","SPARES ORDERED AND CONNECTED ON BOARD FOR RENEWAL."]
[null,null,null,null,11335,"26_4 Apr 2020 1:06:47 PM","2020-03-18","Breakdown","Ship Staff","Ship Staff Insp.","Fresh Water Generator sea water line leaking at various Locations.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.31","Very High","","","All leaking pipe lines renewed with fabricated new lines.","2020-03-25","","Completed","2020-03-24","No","No","No","Internal"]
[null,null,null,null,11334,"26_29 Mar 2020 2:39:43 AM","2020-03-20","Defect","Ship Staff","Ship Staff Insp.","Main Steam Pipeline section aft of Midship crane found leaking.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","","","","","Pipeline section removed and transfered to Engine room workshop, Fabricated New section and replaced old leaking section.","2020-03-22","","Completed","2020-03-22","No","No","No","Internal"]
[null,null,null,null,4154,"26_2019-10-24 19:55:33.000","2020-03-30","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Exhaust truncking below the EGB having leak","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.19","Very High","","","Economizer gas leak, permanent repair carried out.","2020-07-30","","Completed","2020-05-26","Yes","No","No","Internal","Job to be completed in DD."]
[null,null,null,null,11328,"26_4 Apr 2020 3:39:49 PM","2020-03-30","Breakdown","Ship Staff","Ship Staff Insp.","Fwd LT Cooler Sea Water outlet line leaking","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.31","Very High","","","New pipe line fabrication in progress.","2020-04-30","","Completed","2020-04-30","No","No","No","Internal","PIPELINE IS FABRICATED AS PER WEEKLY REPORT, PLEASE CLOSE THE OBSERVATION. SUGGEST TO MAKE ONE SPARE/STANDBY ADDITIONAL OUTLET LINE SECTION."]
[null,null,null,null,11326,"26_2020-04-03 2:37:42 AM","2020-03-31","Defect","Ship Staff","Ship Staff Insp.","Main Steam Pipeline section at 4 W COT found leaking.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","","","","","Pipeline Section removed and transfered to Engine room workshop for fabricating New Pipline.","2020-04-20","","Completed","2020-04-15","No","No","No","Internal","PIPELINE IS RENEWED AS PER WEEKLY REPORT, PLEASE UPDATE THE RECORD."]
[null,null,null,null,11327,"26_2020-04-04 9:32:16 AM","2020-04-01","Defect","Ship Staff","Ship Staff Insp.","Port and Starboard gangway spring for pawl found broken.","Deck - Machinery","Structural Condn. / WT integrity ","Equipment Related","","","","","As no Spares available onboard, New Spring fabricated and replaced. Requisition Raised","2020-05-31","AQUA200053","Completed","2020-04-30","No","No","No","Internal","SPARES ORDERED AS PER AQUA200053. WILL BE CONNECTED TO VESSEL ONCE READY. \nHOWEVER ACTION TAKEN BY STAFF IS SUFFICIENT AND OBSERVATION IS CONSIDERED CLOSED."]
[null,null,null,null,12177,"26_2020-05-23 11:04:35 AM","2020-04-13","Defect","Ship Staff","Ship Staff Insp.","Slop (S) Tank Cleaning Machine found not operational.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","Worn out parts replaced with newly received spares.","2020-05-31","","Completed","2020-05-18","No","No","No","Internal"]
[null,null,null,null,10809,"26_2020-01-26 6:15:41 AM","2020-04-15","Defect","Ship Staff","Ship Staff Insp.","Hose Handling crane Luffing Cylinder Seal Leaking.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.73","Medium","","","Seal to be changed in Dry Dock","2020-07-30","","Completed","2020-08-30","Yes","No","No","Internal","JOB COMPLETED IN DD @SEMBCORP ADMIRALTY YARD."]
[null,null,null,null,19039,"26_30 Apr 2021 8:14:17 PM","2020-04-15","Defect","Ship Staff","Ship Staff Insp.","Hydrants - 4 nos and Foam Monitor - 2 nos found leaking during normal inpections\t","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.38","High","","","Hydrants and Foam Monitors opened / Overhauled / Cleaned and Pressure test carried out. No leaks Observed","2021-07-15","","Completed","2021-04-21","No","No","No","Internal"]
[null,null,null,null,4135,"26_2019-10-24 05:22:01.000","2020-04-30","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Few of the bunker/ballast tanks sounding caps are not fitting tightly; repairs needed to redress threads for better fit.","Miscellaneous","Cargo / Ballast Systems","Equipment Related","10.35","Very High","","","Temporary repairs with soft patch work done.Necessary permanent repairs to be carried out in DD.","2020-07-30","","Completed","2020-08-30","Yes","No","No","Internal","SOUNDING CAPS RENEWED."]
[null,null,null,null,9726,"26_15 Jan 2020 7:11:46 PM","2020-04-30","Observation","Ship Staff","Ship Staff Insp.","Provision crane limit switchs found not working.","Deck - Machinery","Eng. / Strg. Comp.","Equipment Related","10.28","Low","","","Received spare at singapore 08.05.20. in progress","2020-07-30","AQUA205016","Completed","2020-08-30","Yes","No","No","Internal","Limit switches were ordered and connected on board.  Renewed during DD @Sembcorp Shipyard."]
[null,null,null,null,9727,"26_15 Jan 2020 7:14:13 PM","2020-04-30","Observation","Ship Staff","Ship Staff Insp.","Hose handling crane luffing limit switch found erratic","Deck - Machinery","Eng. / Strg. Comp.","Equipment Related","8.73","Medium","","","Tourbleshooting in progress","2020-07-30","","Completed","2020-08-30","Yes","No","No","Internal","Complete health check up completed by crane specialist and completed repairs during vessel docking @Sembcorp Admiralty shipyard."]
[null,null,null,null,10818,"26_2020-01-30 11:35:51 AM","2020-05-01","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Stub pieces on the cargo lines for Air blowing connection are thinned down and rusted\n\nrequire renewal","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","","","","","Presently soft patched with Devcon carried out.","2020-07-31","","Completed","2020-08-30","Yes","No","No","Internal","ALL WORN OUT STUB PIECES RENEWED DURING DD @SEMBCORP ADMIRALTY YARD."]
[null,null,null,null,12178,"26_2020-05-23 11:13:02 AM","2020-05-14","Defect","Ship Staff","Ship Staff Insp.","Aft Spring Mooring winch both Brake bands found badly corroded and thinned down.","Deck - Mooring Machinery","Mooring","Equipment Related","","","","","repaired with hot work","2020-05-21","","Completed","2020-05-19","No","No","No","Internal"]
[null,null,null,null,10814,"26_2020-01-30 11:57:03 AM","2020-05-15","Critical Equipment","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Cargo lines flanges and various line flanges hydro blasting to be carried out.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","","","","","Hydro Blasting Machine Hose and Union coupling ordered to reach to Manifold area.","2020-08-15","AQUA200006","Completed","2020-08-30","No","No","No","Internal","JOB COMPLETED DURING DD @SEMBCORP ADMIRALTY YARD SINGAPORE."]
[null,null,null,null,11329,"26_2020-03-17 1:14:13 PM","2020-05-15","Defect","Ship Staff","Ship Staff Insp.","Slop (P) Cargo Pump, Cargo Seal leaking.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","Seal to be changed.","2020-08-15","","Completed","2020-08-30","Yes","No","No","Internal","JOB COMPLETED DURING DD @SEMBCORP ADMIRALTY YARD."]
[null,null,null,null,12176,"26_5 Jun 2020 11:00:51 AM","2020-05-18","Observation","Ship Staff","Ship Staff Insp.","Fixed Gas Dtection system Detector Fault Alarm Received on Main control panel.","Miscellaneous","Cargo / Ballast Systems","Equipment Related","","","","","Troubleshooting carried out, found detector fault, message sent to office, waiting for office reply.","2020-06-30","","Completed","2020-06-20","No","No","No","Internal","NEW GAS DETECTOR, VACUUM PUMP DIAPHRAGM, FLOW-METER SUPPLIED TO VESSEL, STAFF RENEWED THESE COMPONENTS AND UNIT IS FUNCTIONING IN ORDER."]
[null,null,null,null,12179,"26_5 Jun 2020 12:37:44 PM","2020-05-20","Observation","Ship Staff","Ship Staff Insp.","No.1 Boiler Water Circulating pump shaft sleeve leaking","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","No.1 Boiler Water Circulating pump Mechanical seal and shaft sleeve renewed.","2020-06-10","","Completed","2020-05-31","No","No","No","Internal"]
[null,null,null,null,12180,"26_5 Jun 2020 12:40:58 PM","2020-05-24","Observation","Ship Staff","Ship Staff Insp.","Main Engine Back Wash Filter change over unit leaking","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Main Engine Back Wash Filter change over unit overhauled, all O rings and bearings renewed","2020-06-05","","Completed","2020-06-01","No","No","No","Internal"]
[null,null,null,null,12174,"26_5 Jun 2020 5:51:18 PM","2020-05-26","Defect","Ship Staff","Ship Staff Insp.","Starboard Anchor Cable 6 Links bent and 1 link found elongated between No7 & No.8 Kenter Shackle.","Deck - Mooring Machinery","Mooring","Equipment Related","","","","","Requsition raised for 1 shackle and 2 kenter shackle, same to be renewed during drydock.","2020-08-30","","Completed","2020-08-30","No","No","No","Internal","CHAIN LENGTHS 7,8 AND 9 FOR STARBOARD ANCHOR CABLE  RENEWED DURING DD @SEMBCORP ADMIRALTY YARD SINGAPORE."]
[null,null,null,null,17152,"26_Fri Jan 15 2021 05:34:46 GMT+0000","2020-06-12","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","FIRE LINE BRANCHES TO INSPECT THROUGHLY AND WEAK SECTIONS TO RENEW.","Deck - Pipe / Fittings","Emgcy. Systems","External Factors","","","","","ALL LINES WERE INSPECTED AND ONE BRANCH LINE ONLY RENEWED.","2020-08-31","","Completed","2020-08-15","No","No","No","Internal","NOTED."]
[null,null,null,null,17153,"26_Fri Jan 15 2021 05:39:34 GMT+0000","2020-06-12","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","STEAM LINES REPAIRS ON DECK TO CONTINUE. ALL REPAIRED LINES MUST BE COATED AT LEAST WITH 3-4 COATS FOR DURABILITY.","Deck - Pipe / Fittings","Cargo / Ballast Systems","External Factors","","","","","VARIOUS STEAM LINES RENEWED AND COATING OF LINES CARRIED OUT AFTER RENEWALS.","2020-08-31","","Completed","2020-08-31","No","No","No","Internal","THIS IS CONTINUOUS PROCESS AND"]
[null,null,null,null,17154,"26_Fri Jan 15 2021 05:42:12 GMT+0000","2020-06-12","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","GREASING POINTS TO BE MARKED ON ALL MOORING FITTINGS AND MONTHLY SCHEDULE TO BE PREPARED TO COVER GREASING AT ALL POINTS.","Deck - Mooring Machinery","Mooring","Human Error","","","","","GREASING POINTS MARKED.","2020-06-30","","Completed","2020-06-30","No","No","No","Internal","GREASING POINTS MARKED."]
[null,null,null,null,17155,"26_Fri Jan 15 2021 05:46:13 GMT+0000","2020-06-12","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","EACH AND EVERY VALVE ON DECK OF CARGO LINES, HYDRAULIC LINES, STEAM LINES, FIRE LINES, FOAM LINE TO CHECK FOR OPERATION AND ENSURE OPERATIONABILITY OF EACH ONE.","Deck - Pipe / Fittings","General Appearance","External Factors","","","","","ALL VALVES CHECKED AND COATED AS PER COLOUR CODE.","2020-06-30","","Completed","2020-06-30","No","No","No","Internal","NOTED WORK CARRIED OUT."]
[null,null,null,null,17156,"26_Fri Jan 15 2021 05:55:29 GMT+0000","2020-06-12","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","BAY AREA PAINTING WORK- FOCUS TO BE PROVIDED TO ENSURE ALL AREAS, PIPEWORK, SUPPORTS, U CLAMPS OF EVERY BAY ARE COVERED DURING PAINTING. LONGITUDINAL UNDERNEATH SECTIONS MUST BE DERUSTED AND COATED WELL DURING THE PROCESS. TO RAISE REQUISITION FOR DFT GAUGE.","Deck - Pipe / Fittings","General Appearance","External Factors","","","","","AREAS OF ATTENTION PAINTED.","2020-06-30","","Completed","2020-06-30","No","No","No","Internal","NOTED."]
[null,null,null,null,17157,"26_Fri Jan 15 2021 06:02:01 GMT+0000","2020-06-12","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","UPPER DECK SHELTER AREA INSIDE AND OUTSIDE NEED GOOD TOUCH UP. AREA TO SPOT DERUST AND PAINT FROM INSIDE AND OUTSIDE.","Miscellaneous","General Appearance","External Factors","","","","","AREAS TOUCHED UP.","2020-08-31","","Completed","2020-08-06","No","No","No","Internal","IT WILL BE NEEDED TO PAINT FULL OF ACCOMODATION IN NEAR FUTURE FOR BETTER COSMETIC APPEARANCE."]
[null,null,null,null,17158,"26_Fri Jan 15 2021 06:11:32 GMT+0000","2020-06-12","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","HYDRUALIC LINES ON DECK TO BE INSPECTED THROUGHLY AND RENEW WEAKER SECTIONS.","Deck - Pipe / Fittings","Eng. / Strg. Comp.","External Factors","","","","","ALL HYDRAULIC LINES THICKNESS GAUGING DONE. THINNED DOWN SECTIONS RENEWED DURING VESSEL'S DOCKING IN AUGUST AT SINGAPORE.","2020-08-31","","Completed","2020-08-29","No","No","No","Internal","ALL HYDRAULIC LINES TO BE MONITORTED AND PROTECTED FROM CORROSION."]
[null,null,null,null,17159,"26_Fri Jan 15 2021 06:17:26 GMT+0000","2020-06-12","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","STEAM RETURN LINE EXPANSION JOINTS TO RENEW WHERE DISTANCE PIECES FITTED INSTEAD.","Deck - Pipe / Fittings","Cargo / Ballast Systems","External Factors","","","","","EXPANSION JOINTS FITTED BACK.","2020-06-25","","Completed","2020-06-22","No","No","No","Internal","NOTED."]
[null,null,null,null,17160,"26_Fri Jan 15 2021 07:42:18 GMT+0000","2020-06-12","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ALL BUNKER TANK VENTS ON DECK, LO/HO/DO BUNKER MANIFOLDS, SLUDGE/BILGE/SEWAGE MANIFOLDS TO CHECK AND CARRY OUT REQUIRED COSMETIC MAINTENANCE. TO CARRY OUT STENCILING FOR EASY IDENTIFICATION.","Deck - Pipe / Fittings","General Appearance","External Factors","","","","","ALL MANIFOLDS, VENTS CHECKED, SERVICED AND FINALLY STENCILED.","2020-06-30","","Completed","2020-06-30","No","No","No","Internal","NOTED WORK CARRIED OUT."]
[null,null,null,null,17207,"26_Fri Jan 15 2021 07:47:36 GMT+0000","2020-06-12","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","WINDLASS BRAKE LINKAGES TO BE ADJUSTED PROPERLY SO THAT UPPER AND LOWER BRAKE BANDS HAVE UNIFORM WEAR.","Deck - Mooring Machinery","Mooring","External Factors,Human Error","","","","","ADJUSTMENTS CARRIED OUT FOR ALL WINCHES.","2020-06-30","","Completed","2020-06-30","No","No","No","Internal","NOTED."]
[null,null,null,null,17208,"26_Fri Jan 15 2021 07:59:17 GMT+0000","2020-06-12","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","CHIEF OFFICER TO TRAIN CREW FOR QUALITY SURFACE PREPERATION AS WELL AS PAINT APPLICATION.","Miscellaneous","Crew Management","Human Error","","","","","TRAINING SESSION CARRIED OUT WITH DCK/ER TEAM AND BRIEFED ON PAINTING APPLICATIONS AND SURFACE PREPARATIONS.","2020-07-31","","Completed","2020-07-15","No","No","No","Internal","THIS TYPE OF TRAINING TO BE CONDUCTED WHENEVER THERE IS MAJOR CREW CHANGE IN ORDER TO REFRESH ON THE TOPIC OF PAINTING."]
[null,null,null,null,17209,"26_Fri Jan 15 2021 08:03:31 GMT+0000","2020-06-12","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ALL REDUCERS WERE RENEWED IN LAST ONE YEAR, COAT THEM INSIDE/OUSIDE AND ENSURE THAT JOINT SURFACES ARE GREASED AND NOT ALLOWED TO CORRODE. ALSO THEY MUST BE STOWED/PROTECTED WITH TARPAULIN CANVAS.","Deck - Pipe / Fittings","General Appearance","Human Error","","","","","ALL REDUCERS WERE CLEANED, COATED AND STOWED SAFELY.","2020-06-30","","Completed","2020-06-30","No","No","No","Internal","REDUCERS MUST BE MAINTAINED IN GOOD ORDER."]
[null,null,null,null,17241,"26_Fri Jan 15 2021 08:41:12 GMT+0000","2020-06-12","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","WINCH BRAKE CYLINDER FEW FLEXIBLE HYDRAULIC HOSES NEED TO BE RENEWED, TO COMPLETE THE JOB ALONG WITH BRAKE TESTING.","Deck - Mooring Machinery","Mooring","External Factors","","","","","ALL FLEXIBLE PIPES HAVE BEEN RENEWED. BRAKES TEST CARRIED OUT FOR ALL WINCHES; SATISFACTORY.","2020-07-12","","Completed","2020-07-06","No","No","No","Internal","NOTED WORK CARRIED OUT."]
[null,null,null,null,17242,"26_Fri Jan 15 2021 08:47:55 GMT+0000","2020-06-12","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","DECK PIPELINES HAVE FEW BLISTER AND SPOT RUST MARKS, TO DERUST THEM AND COAT.","Deck - Pipe / Fittings","General Appearance","External Factors","","","","","THINNED DOWN LINES RENEWED. OTHER PIPELINES TOUCH UP WORK CARRIED OUT FOR CORROSION PROTECTION.","2020-08-31","","Completed","2020-08-29","No","No","No","Internal","CORROSION PROTECTION AND MONITORING IS CONTINOUS PROCESS AND TO BE FOLLOWED UP DUE DILIGENTLY."]
[null,null,null,null,17243,"26_Fri Jan 15 2021 09:25:26 GMT+0000","2020-06-12","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","TO VERIFY CONTROL AIR DRYER CONDITION AND REPORT TO OFFICE. ENSURE DAILY AIR BOTTLE DRAINING. AUTO DRAINS TO OVERHAUL FOR CORRECT FUNCTIONING.","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related","","","","","CHECKED AND ENSURED AUTO FUNCTIONING OF UNIT.","2020-06-30","","Completed","2020-06-28","No","No","No","Internal","AIR DRIER MUST BE WORKING SATISFACTORY ALL THE TIME; THIS IS VITAL FOR SATISFACTORY FUNCTIONING OF ALL PNEUMATIC COMPONENTS ON BOARD."]
[null,null,null,null,17244,"26_Fri Jan 15 2021 09:29:51 GMT+0000","2020-06-12","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ONCE VRCS SPARE ARE RECEIVED, TO CARRY OUT OVERHAUL OF LEAKING 2P CARGO VALVE.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","","","","","2P CARGO VALVE OVERHAULED.","2020-06-30","","Completed","2020-06-24","No","No","No","Internal","NOTED."]
[null,null,null,null,17245,"26_Fri Jan 15 2021 09:36:02 GMT+0000","2020-06-12","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","AUX BOILER AUTO OPERATION – PARAMETERS NEED TO BE TUNED. PLEASE REVERT ISSUES; WE WILL LIAISE WITH MAKERS TO GET SUFFICIENT DATA.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","ALL LINKAGES GREASED AND ROUTINES CARRIED OUT.","2020-07-31","","Completed","2020-07-15","No","No","No","Internal","NOTED."]
[null,null,null,null,17246,"26_Fri Jan 15 2021 09:40:58 GMT+0000","2020-06-12","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ALL SIGNAL LIGHT COLUMNS TO VERIFY FOR CORRECT FUNCTIONING AND REPORT TO OFFICE.","Elect. Mach. & Equip.","Emgcy. Systems","Equipment Related","","","","","ALL SIGNAL LIGHT COLUMNS CHECKED AND WORKING SATISFACTORY.","2020-06-30","","Completed","2020-06-22","No","No","No","Internal"]
[null,null,null,null,17247,"26_Fri Jan 15 2021 09:44:55 GMT+0000","2020-06-12","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","LT COOLER STAIN MARKS TO CLEAN AND RECTIFY LEAKS IF ANY.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Human Error","","","","","LT COOLER ALL LINES CLEANED UP AND CHECKED FOR INTEGRITY; FOUND IN GOOD ORDER.","2020-06-15","","Completed","2020-06-15","No","No","No","Internal","NOTED."]
[null,null,null,null,17248,"26_Fri Jan 15 2021 09:50:05 GMT+0000","2020-06-12","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","IGG HMI TOUCH SCREEN PANEL IS NOT FUNCTIONING, NEW PANEL IS ORDERED (HAVING 2 MONTHS DELIVERY PERIOD). ONCE READY WILL BE CONNECTED.","Inert Gas","Cargo / Ballast Systems","Equipment Related","","","","","IGG OPERATION WAS UNITERRUPTED AND WAS CARRIED OUT IN AUTO MODE USING SWITCH CONTROLS. IGG SCREEN ON RECEIPT RENEWED.","2020-08-30","","Completed","2020-08-29","No","No","No","Internal","NOTED WORK CARRIED OUT."]
[null,null,null,null,17250,"26_Fri Jan 15 2021 10:42:21 GMT+0000","2020-06-12","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ME AND AE FLOWMETER TO RENEW ONCE RECEIVED ON BOARD.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Flowmeters renewed. During the time digital once were out of use, mechanical flowmeters were in place for getting fuel consumptions.","2020-07-15","","Completed","2020-07-15","No","No","No","Internal","Noted."]
[null,null,null,null,17251,"26_Fri Jan 15 2021 10:46:07 GMT+0000","2020-06-12","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ILLUMINATION IN EROOM HAS DROPPED. SUGGEST TO CLEAN ALL LIGHT COVERS AND RENEW ALL FUSED BULBS.","Elect. Mach. & Equip.","General Appearance","Human Error","","","","","Light covers cleaned. LEDs renewed at few platforms as required.","2020-07-15","","Completed","2020-07-15","No","No","No","Internal"]
[null,null,null,null,17252,"26_Fri Jan 15 2021 10:49:15 GMT+0000","2020-06-12","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ANTI SPLASHING TAPES MISSING FROM ME FUEL INJECTOR JOINTS.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Human Error","","","","","Anti splashing tapes put in place wherever missing.","2020-06-30","","Completed","2020-06-25","No","No","No","Internal","Noted and Compliance is must."]
[null,null,null,null,17253,"26_Fri Jan 15 2021 11:16:33 GMT+0000","2020-06-12","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ER BULKHEADS TO SOAPWASH (FROM TOP TO BOTTOM).\nSTEERING ROOM TO SOAPWASH AND PAINT WHEREVER NECESSARY.\nALL MACHINERIES TO SOAPWASH (NO PAINTING).\nALL MOTORS TO SOAPWASH (BY ETO).","Miscellaneous","General Appearance","Human Error","","","","","Soapwash carried out for various areas, motors as necessary.","2020-07-31","","Completed","2020-07-30","No","No","No","Internal"]
[null,null,null,null,17254,"26_Fri Jan 15 2021 11:22:02 GMT+0000","2020-06-12","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","SPARES INVENTORY TO UPDATE IN PAL","E/R - Aux. Mach.,Miscellaneous","Eng. / Strg. Comp.","Human Error","","","","","Spares inventory updated in PAL.","2020-08-31","","Completed","2020-08-07","No","No","No","Internal","This is continuous job ."]
[null,null,null,null,17255,"26_Fri Jan 15 2021 11:25:39 GMT+0000","2020-06-12","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ALL PRESSURE AND TEMPERATURE GAUGES TO CHECK IN EROOM, DECK. NON OPERATIONAL ONES TO RENEW.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","This is continuous process and regular monitoring is to ensure flawless operation.","2020-07-07","","Completed","2020-07-15","No","No","No","Internal","Compliance must."]
[null,null,null,null,17100,"26_Thu Jan 14 2021 02:44:56 GMT+0000","2020-06-12","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","MAGNETIC COMPASS DEVIATION UPTO 5 DEG IS ACCEPTABLE, CHECK PRESENT DEVIATION AND CORRECT IT VIA SHORE SERVICE TEAM ENGAGED.","Navigation - Others","Navigation","Equipment Related","","","","","REMOTE CALIBRATION DONE WITH THAWE MARINE.","2020-07-15","","Completed","2020-07-15","No","No","No","Internal","MAGNETIC COMPASS DEVIATION TO MONITOR REGULARLY ."]
[null,null,null,null,17150,"26_Fri Jan 15 2021 04:22:28 GMT+0000","2020-06-12","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","MAGNETIC COMPASS DEVIATION UPTO 5 DEG IS ACCEPTABLE, CHECK PRESENT DEVIATION AND CORRECT IT VIA SHORE SERVICE TEAM ENGAGED.","Navigation - Others","Navigation","Equipment Related","","","","","REMOTE CALIBRATION COMPLETED WITH THAWE MARINE.","2020-07-15","","Completed","2020-07-15","No","No","No","Internal","NOTED."]
[null,null,null,null,17151,"26_Fri Jan 15 2021 04:28:14 GMT+0000","2020-06-12","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","MUSHROOM VENTS ON DECK –STEEL PLATING HAS THINNED DOWN. DISMANTLE COMPLETE VENT AND CARRY OUT STEEL REPAIRS IN ER WORKSHOP. FIT BACK AFTER SUFFICIENT PAINT COATS.","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","External Factors","","","","","SUBJECT VENTS CHECKED DURING VESSEL DOCKING AND SUBJECT STEEL PLATING RENEWED. VENT COATED AND FIXED BACK.","2020-08-31","","Completed","2020-08-29","No","No","No","Internal","JOB COMPLETED DURING DRYDOCK."]
[null,null,null,null,16687,"26_5 Jan 2021 11:34:23 AM","2020-06-13","Observation","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","Navigating officer not familiar with SCAMIN when to be OFF for apprasial plan, open in execution state as per NP232 (page 80)","Navigation - ECDIS","Navigation","Knowledge Based","4.14","Very High","","","The cocerned officer was made to redo  type specific ECDIS familirization with company form12.01.32.021.01 - ship specific ECDIS familiarizaion and Audit checklist. Same circulated for fleet awareness.","2020-06-30","","Completed","2020-06-15","No","No","No","External"]
[null,null,null,null,16688,"26_5 Jan 2021 12:16:17 PM","2020-06-13","Observation","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","No record inside fixed deck foam frefighting system for 5 yearly internal inspection maintenance of controlled valves by trained personnel and hyper mist system for engine room with regard to 5 yearly internal inspection / overhaul of all control & section valves.","LSA / FFA","Safety / LSA / FFA","Inappropriate Procedure","5.35","Medium","","","Vessel class Bureau veritas has confirmed that the 5 yearly service and maintenance has been carried out during docking related repairs, report sent from class for same. ","2020-06-30","","Completed","2020-06-16","No","No","No","External"]
[null,null,null,null,16690,"26_5 Jan 2021 11:39:49 AM","2020-06-13","Observation","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","Forward and Midship portside draft marks from 10.70 mtr. not legible","Hull & Tanks","General Appearance","External Factors","11.2","Medium","","","Draft mark painted when vessel at Tanjung Pelepas","2020-06-30","","Completed","2020-06-17","No","No","No","External"]
[null,null,null,null,16689,"26_5 Jan 2021 1:21:11 PM","2020-07-07","Non Conformity","PSC Insp.","Flag State Insp.","Crew not releived as per terms of contract","Miscellaneous","MLC Related","External Factors","","","","","Due to COvid  19 panadmeic, severe restriction for crew change implemented in majority ports. However necessary schedule for sam arranged for timely relief.","2020-10-07","","Completed","2020-09-13","No","No","No","External"]
[null,null,null,null,17919,"26_19 Feb 2021 5:56:46 PM","2020-08-02","Observation","Ship Staff","Ship Staff Insp.","Telegraph order printer on wheel house not operational","E/R - Main Engine,Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","Requisition raised\n\nReplaced by an old & used printer received by vessel - working satisfactory although few moving parts have been noted to be rusted.","2021-02-01","AQUA200123","Completed","2021-01-04","No","No","No","Internal"]
[null,null,null,null,17049,"26_Wed Jan 13 2021 05:31:25 GMT+0000","2020-08-29","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","TO IMPART TRAINING TO BOSUN AND ABs AND ONLY ALLOW THEM FOR HOSE HANDLING/PROVISION CRANE OPERATION. \n\nONE OFFICER (BASED ON DEPARTMENTAL WORK) MUST BE PRESENT DURING EVERY CRANE OPERATION TO OBSERVE CRANE MOVEMENTS AND SAFETY.","Deck - Machinery","Cargo / Ballast Systems","Inappropriate Procedure","","","","","TO IMPART TRAINING TO BOSUN AND ABs AND ONLY ALLOW THEM FOR HOSE HANDLING/PROVISION CRANE OPERATION. \n\nONE OFFICER (BASED ON DEPARTMENTAL WORK) MUST BE PRESENT DURING EVERY CRANE OPERATION TO OBSERVE CRANE MOVEMENTS AND SAFETY.","2020-09-15","","Completed","2020-09-10","No","No","No","Internal","TRAINING AND COMPLIANCE MUST"]
[null,null,null,null,17050,"26_Wed Jan 13 2021 05:36:19 GMT+0000","2020-08-29","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","HYDRUALIC LINES ON DECK – WEAKER/THINNER PIPELINES WERE RENEWED DURING RECENT DOCKING.  FOR REMAINING PIPELINE STRENGTHENING WORK NEED TO BE CARRIED OUT; ALL PITTED AREAS (IN WAY OF PIPE CLAMPS) SURFACE TO BE PREPARED FOR BELZONA APPLICATION. WE HAVE SUPPLIED 3 TINS OF BELZONA, THIS TO BE USED TO FILL UP PITTED HOLES AND THEN APPLY FEW COATS OF PRIMER/FINAL COAT.","Deck - Pipe / Fittings","Cargo / Ballast Systems","External Factors","","","","","ALL PITTED AREAS (IN WAY OF PIPE CLAMPS) SURFACE TO BE PREPARED FOR BELZONA APPLICATION. WE HAVE SUPPLIED 3 TINS OF BELZONA, THIS TO BE USED TO FILL UP PITTED HOLES AND THEN APPLY FEW COATS OF PRIMER/FINAL COAT.","2020-11-30","","Completed","2020-11-15","No","No","No","Internal","CARRY OUT NECESSARY IMPROVISATION WORK TO INCREASE PIPE LIFE."]
[null,null,null,null,17051,"26_Wed Jan 13 2021 05:39:58 GMT+0000","2020-08-29","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","WATER BALLAST TANKS PENDING LADDERS RENEWAL TO COMPLETE-\n1S - 1 Ladder 2nd Level.\n2S – 4 Ladders 1st and 2nd Level.\n3P – 1 Ladder 2nd Level.\n3S – 2 Ladders 2nd Level.\n4P – 2 Ladders at 2nd and 3rd Level.\n4S – 1 Ladder 3rd Level.","Hull & Tanks","Cargo / Ballast Systems","External Factors","","","","","WATER BALLAST TANKS PENDING LADDERS RENEWAL TO COMPLETE-\n1S - 1 Ladder 2nd Level.\n2S – 4 Ladders 1st and 2nd Level.\n3P – 1 Ladder 2nd Level.\n3S – 2 Ladders 2nd Level.\n4P – 2 Ladders at 2nd and 3rd Level.\n4S – 1 Ladder 3rd Level.","2020-12-31","","Completed","2020-12-15","No","No","No","Internal","NOTED THAT LADDERS RENEWAL JOB IS COMPLETED. ALSO TANK AREAS COATING REPAIRS HAVE BEEN COMPLETED."]
[null,null,null,null,17052,"26_Wed Jan 13 2021 05:49:28 GMT+0000","2020-08-29","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ALL WBT TANK VENTS ON DECK WERE ALREADY CHECKED IN PAST AND WERE REQUIRING MAINTENANCE. REQUIRED CONSUMABLES (FLOATS, GASKETS, NUT/BOLTS) WERE SUPPLIED LAST CALL SINGAPORE. TO COMPLETE JOB THROUGHLY.","Hull & Tanks","Cargo / Ballast Systems","Inappropriate Procedure","","","","","ALL WBT TANK VENTS ON DECK WERE ALREADY CHECKED IN PAST AND WERE REQUIRING MAINTENANCE. REQUIRED CONSUMABLES (FLOATS, GASKETS, NUT/BOLTS) WERE SUPPLIED LAST CALL SINGAPORE. TO COMPLETE JOB THROUGHLY.","2020-09-30","","Completed","2020-09-15","No","No","No","Internal","NOTED THAT WBT TANK VENTS NOW FITTED WITH NEW GASKETS, FLAOTS WHEREVER NECESSARY."]
[null,null,null,null,17053,"26_Wed Jan 13 2021 06:03:02 GMT+0000","2020-08-29","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","MUSHROOM VENTS ON DECK –STEEL PLATING HAS THINNED DOWN. DISMANTLE COMPLETE VENT AND CARRY OUT STEEL REPAIRS IN ER WORKSHOP. FIT BACK AFTER SUFFICIENT PAINT COATS.","Deck - Pipe / Fittings","General Appearance","Inappropriate Procedure","","","","","VENT STEEL PLATING TO CHECK AND ONLY VENT'S PLATING WHICH ARE THINNED DOWN TO RENEW. OR OTHERWISE, JUST COAT VENTS FROM INSIDE.","2020-11-29","","Completed","2020-09-15","No","No","No","Internal","NOTED THAT ALL VENTS CHECKED AND CONDITION FOUND OK."]
[null,null,null,null,17054,"26_Wed Jan 13 2021 06:07:44 GMT+0000","2020-08-29","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","FIRE LINE BRANCHES TO INSPECT THROUGHLY AND WEAK SECTIONS TO RENEW.","Deck - Pipe / Fittings","Safety / LSA / FFA","Inappropriate Procedure","","","","","FIRE LINE BRANCHES INSPECTED AND ARE APPEARED IN HEALTHY CONDITION.","2020-09-15","","Completed","2020-09-15","No","No","No","Internal","NOTED THAT FIRE LINE BRANCHES ARE OK."]
[null,null,null,null,17055,"26_Wed Jan 13 2021 06:13:35 GMT+0000","2020-08-29","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","STEAM LINES REPAIRS ON DECK TO CONTINUE.   SUGGEST TO PLAN RENEWALS ON WEEKLY BASIS TO AVOID LAST MINUTE REPAIRS.                                                                                                                ALL REPAIRED LINES MUST BE COATED AT LEAST WITH 3-4 COATS WITH SPECIAL HIGH TEMPERATURE PAINT FOR DURABILITY.","Deck - Pipe / Fittings","Cargo / Ballast Systems","External Factors","","","","","VARIOUS STEAM LINES AND BRANCHES WHICH WERE THINNED DOWN HAVE BEEN RENEWED.","2020-11-30","","Completed","2020-11-30","No","No","No","Internal","NOTED ON ALL STEAM LINES RENEWALS. LINES NEED TO BE CONTINUOUSLY MONITORED FOR LEAKS."]
[null,null,null,null,17056,"26_Wed Jan 13 2021 06:19:17 GMT+0000","2020-08-29","Defect,Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","BAY AREA PAINTING WORK- FOCUS TO BE PROVIDED TO ENSURE ALL AREAS, PIPEWORK, SUPPORTS, U CLAMPS OF EVERY BAY ARE COVERED DURING PAINTING. LONGITUDINAL UNDERNEATH SECTIONS MUST BE DERUSTED AND COATED WELL DURING THE PROCESS.","Deck - Pipe / Fittings","General Appearance","Inappropriate Procedure","","","","","ALL NECESSARY AREAS HYDROBLASTED, PREPARED AND COATED.","2020-11-30","","Completed","2020-11-30","No","No","No","Internal","FABRIC MAINTENANCE IS CONTINOUS PROCESS AND STAFF TO DUE DILIGENTLY FOLLOW MONITORING PROCESS WITH NECESSARY ACTIONS."]
[null,null,null,null,17057,"26_Wed Jan 13 2021 06:24:07 GMT+0000","2020-08-29","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ALL REDUCERS WERE RENEWED IN LAST ONE YEAR, COAT THEM INSIDE/OUSIDE AND ENSURE THAT JOINT SURFACES ARE GREASED AND NOT ALLOWED TO CORRODE. ALSO THEY MUST BE STOWED/PROTECTED WITH TARPAULIN CANVAS.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Inappropriate Procedure","","","","","ALL REDUCERS DERUSTED, PAINTED AND NOW STOWED WITH TARPAULIN CANVAS.","2020-11-30","","Completed","2020-11-30","No","No","No","Internal","NOTED."]
[null,null,null,null,17058,"26_Wed Jan 13 2021 06:36:53 GMT+0000","2020-08-29","Defect,Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","WATER BALLAST TANKS ARE HEAVILY CORRODED AND NEED TO START TANK COATING UPGRADE PROJECT. FOR THIS PROJECT, WE WILL HAVE 2 BLASTERS (RIDING TEAM) PLACED ON BOARD AT SINGAPORE ONCE COVID RESTRICTIONS ARE OFF. THEY WILL SAIL ON BOARD AND COMPLETE ONE BY ONE ALL BALLAST TANKS COATING MAINTENANCE.","Hull & Tanks","General Appearance","Inappropriate Procedure","","","","","WATER BALLAST TANKS COATING UPGRADATION  JOB STARTED AND COMPLETED FOR MAJORITY OF TOP STRINGER AREAS.","2020-11-30","","Completed","2020-11-30","No","No","No","Internal","PRIORITY AREAS COMPLETED. NOW FOCUS TO SHIFT TO COMPLETE ALL NUKE AND CORNERS AS NECESSARY."]
[null,null,null,null,17059,"26_Wed Jan 13 2021 06:44:39 GMT+0000","2020-08-29","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","DECK PIPELINES HAVE FEW BLISTER AND SPOT RUST MARKS, TO DERUST THEM AND COAT.","Deck - Pipe / Fittings","General Appearance","Inappropriate Procedure","","","","","ALL DECK PIPELINES SPOT DERSUTED AND PAINTED.","2020-11-30","","Completed","2020-11-30","No","No","No","Internal","NOTED."]
[null,null,null,null,17060,"26_Wed Jan 13 2021 07:07:16 GMT+0000","2020-08-29","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","GREASING OF BOTH CRANES TO COMPLETE","Deck - Machinery","Cargo / Ballast Systems","Inappropriate Procedure","","","","","CRANES GREASING COMPLETED.","2020-09-15","","Completed","2020-09-15","No","No","No","Internal","NOTED."]
[null,null,null,null,17061,"26_Wed Jan 13 2021 07:26:36 GMT+0000","2020-08-29","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","GREASING OF CRANE WIRES.","Deck - Machinery","Eng. / Strg. Comp.","Inappropriate Procedure","","","","","CRANE WIRES GREASED AFTER DEPARTURE FROM DD.","2020-09-15","","Completed","2020-09-15","No","No","No","Internal","NOTED."]
[null,null,null,null,17062,"26_Wed Jan 13 2021 07:37:56 GMT+0000","2020-08-29","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","WBT LADDERS RENEWED TO BE COATED WITH PRIMER AND FINAL COATS FOR CORROSION PROTECTION.","Hull & Tanks","Cargo / Ballast Systems","External Factors","","","","","JOB COMPLETED.","2020-09-30","","Completed","2020-09-15","No","No","No","Internal","FOLLOW UP WORK AFTER DD."]
[null,null,null,null,17063,"26_Wed Jan 13 2021 07:40:31 GMT+0000","2020-08-29","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","DECK STELL WORK TO BE COATED WITH PRIMER AND FINAL COATS FOR CORROSION PROTECTION.","Deck - Pipe / Fittings","General Appearance","External Factors","","","","","JOB COMPLETED.","2020-09-30","","Completed","2020-09-15","No","No","No","Internal","FOLLOW UP WORK AFTER DD."]
[null,null,null,null,17064,"26_Wed Jan 13 2021 07:42:40 GMT+0000","2020-08-29","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","FORWARD DRAFT GAUGE PIPE COLD REPAIRS TO COMPLETE.","Hull & Tanks","Cargo / Ballast Systems","External Factors","","","","","COLD REPAIRS COMPLETED.","2020-09-15","","Completed","2020-09-15","No","No","No","Internal","NOTED."]
[null,null,null,null,17065,"26_Wed Jan 13 2021 08:37:04 GMT+0000","2020-08-29","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","VRCS LINES IDENTIFICATION AND TAGGING TO COMPLETE IN FOAM ROOM AS WELL AS ON ACCOMODATION BULKHEAD WHERE IT COMES OUT ON OPEN DECK.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Inappropriate Procedure","","","","","VRCS LINES ARE TAGGED INSIDE VRCS CABINATE.","2020-09-30","","Completed","2020-09-05","No","No","No","Internal","NOTED."]
[null,null,null,null,17066,"26_Wed Jan 13 2021 08:53:23 GMT+0000","2020-08-29","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","AUX ENGINE RESILIENT MOUNTING: FEW RESILIENT MOUNTINGS COULD NOT BE ADJUSTED EVEN THOUGH CLEARANCES ARE BELOW 2MM. \n\nREQUISITION AQUA200106 WAS RAISED AND CONFIRMED FOR SUPPLY FOR NEW RESILIENT MOUNTINGS.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","RESILIENT MOUNTINGS RENEWED AFTER RECEIPT OF SPARES.","2020-11-30","","Completed","2020-11-30","No","No","No","Internal","VIBRATION MONITORING TO BE CARRIED OUT  CONTINUOUSLY."]
[null,null,null,null,17067,"26_Wed Jan 13 2021 08:57:33 GMT+0000","2020-08-29","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ALL BUNKER TANK VENTS ON DECK, LO/HO/DO BUNKER MANIFOLDS, SLUDGE/BILGE/SEWAGE MANIFOLDS TO CHECK AND CARRY OUT REQUIRED COSMETIC MAINTENANCE. TO CARRY OUT STENCILING FOR EASY IDENTIFICATION.","Deck - Pipe / Fittings","General Appearance","Inappropriate Procedure","","","","","ALL VENTS MAINTENANCE COMPLETED.","2020-10-31","","Completed","2020-10-31","No","No","No","Internal","NOTED."]
[null,null,null,null,17068,"26_Wed Jan 13 2021 09:02:50 GMT+0000","2020-08-29","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","IGG REQUIRED MAINTENANCE TO COMPLETE AND MAKE IT FULLY AUTO OPERATIONAL.","Inert Gas","Cargo / Ballast Systems","Equipment Related","","","","","IGG MAINTENANCE CARRIED OUT AND UNIT TESTED OK DURING DISCHARGE AT AUSTRALIA.","2020-09-15","","Completed","2020-09-15","No","No","No","Internal","NOTED."]
[null,null,null,null,17069,"26_Wed Jan 13 2021 09:05:54 GMT+0000","2020-08-29","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","HOSE HANDLING CRANE AND PROVISION CRANE LIMIT SWITCHES OPERATION AND ALL OTHER SAFETIES MUST BE CHECKED ON MONTHLY BASIS; MAKE PMS CHANGE REQUEST ACCORDINGLY.","Deck - Machinery","Eng. / Strg. Comp.","Inappropriate Procedure","","","","","PMS CHANGE REQUEST SENT AND IT INVOLVES NOW MONTHLY CHECKING OF LIMIT SWITCHES.","2020-09-15","","Completed","2020-09-15","No","No","No","Internal","NOTED."]
[null,null,null,null,17070,"26_Wed Jan 13 2021 09:09:32 GMT+0000","2020-08-29","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","PROVISION CRANE SOFT STARTER TO RENEW.\nPROVISION CRANE UP/DOWN LIMITER TO RENEW AND TEST CRANE.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","SOFT STARTER AND LIMITER RENEWED. CRANE OPERATION CHECKED, OK.","2020-09-30","","Completed","2020-09-18","No","No","No","Internal","ALL CRANE SAFETIES MUST BE REGULARLY CHECKED."]
[null,null,null,null,14373,"26_29 Oct 2020 10:35:44 AM","2020-09-03","Observation","Ship Staff","Ship Staff Insp.","VRCS - Line leaking at the break of accommodation.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","To make permanent repair.\n\n\n\nLeak rectified by renewing leaky section.","2020-12-02","","Completed","2020-09-11","No","No","No","Internal"]
[null,null,null,null,17920,"26_19 Feb 2021 6:25:39 PM","2020-09-17","Observation","Ship Staff","Ship Staff Insp.","HFO Service Tank - level sensor for remote display is defective - no spare on board.","Hull & Tanks","Eng. / Strg. Comp.","Equipment Related","","","","","Requisition raised.\n\nReplaced sensor & intermediate junction box using new received supply - working satisfactory.","2021-02-16","AQUA200105","Completed","2021-01-05","No","No","No","Internal"]
[null,null,null,null,14366,"26_28 Oct 2020 11:18:10 AM","2020-09-17","Defect","Ship Staff","Ship Staff Insp.","HFO Service Tank - Level Sensor for remote display is defective","Hull & Tanks","Eng. / Strg. Comp.","Equipment Related","","","","","Requisition already raised.\n\nReplaced defective sensor & junction box by newly received supply - working satisfactory.","2020-12-16","AQUA200105","Completed","2021-01-05","No","No","No","Internal","Sensor will be placed on board soon as spare part now ready to be connected.  After receipt of spare replace it.\n\nNoted sensor renewed and issue is resolved."]
[null,null,null,null,14367,"26_28 Oct 2020 11:21:33 AM","2020-09-17","Observation","Ship Staff","Ship Staff Insp.","ME Turbocharger - exhaust gas inlet temperature not available in ECR alarm monitoring panel - thermocouple defective","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Requisition already raised.\n\nReceived new temperature sensor fitted but reading incorrect. Adjusted span & zero value but on ME at full rpm, the readout jumps from 340 °C to max triggering sensor fail alarm.\n\nR-I convertor renewed but no improvement.\n\non further investigation found the cable from sensor is deteriorated (verified by connecting a spare cable directly).\n\nThe defective cable to be renewed, laid out along the original path and secured; connections made - will monitor upon departure Chittagong.\n\nat ME full rpm, the display at ECR AMS is working normal.","2021-03-16","AQUA200141","Completed","2021-02-25","No","No","No","Internal","Order placed and spare will be connected on board for replacement."]
[null,null,null,null,14368,"26_29 Oct 2020 12:02:41 PM","2020-09-17","Observation","Ship Staff","Ship Staff Insp.","Stern Tube - Fwd bearing temperature displayed as 104 °C & sensor faulty","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","To investigate & troubleshoot.\n\n\n\nOn troubleshooting found the R-I convertor is malfunctioning/defective. Requisition raised.\n\nR-I convertor renewed for both fwd and aft units using new supply - working satisfactory.","2021-03-16","AQUA200218","Completed","2021-01-27","No","No","No","Internal","Clean existing sensor, check cable continuity, check electrical connections. After investigation, revert finding for follow up!\n\nBasis troubleshooting, we have ordered spares and will be connected once ready. Till that period, monitor oil return temperature."]
[null,null,null,null,14374,"26_28 Oct 2020 8:26:32 PM","2020-09-17","Observation","Ship Staff","Ship Staff Insp.","VRCS - deteriorated performance noted for 5/2 valves during operation.","Deck - Machinery","Cargo / Ballast Systems","Equipment Related","","","","","5/2 valves - to renew on deck & operation to confirm during operation.\n\n\n\n5/2 valves replaced by new supply - operation tested & verified.","2020-12-16","","Completed","2020-09-18","No","No","No","Internal"]
[null,null,null,null,14375,"26_28 Oct 2020 8:31:17 PM","2020-09-17","Observation","Ship Staff","Ship Staff Insp.","Prov. Crane - observed deteriorated performance of soft starter and limit switches and malfunction exhibited.","Deck - Machinery","Eng. / Strg. Comp.","Equipment Related","","","","","To renew defective components.\n\n\n\nRenewed soft starter and limit switches","2020-11-26","AQUA205075","Completed","2020-09-17","No","No","No","Internal"]
[null,null,null,null,17921,"26_19 Feb 2021 6:31:08 PM","2020-09-18","Observation","Ship Staff","Ship Staff Insp.","Provision Crane - Limit Switches for slewing operation not functional due to missing operating steel bar.","Deck - Machinery","Eng. / Strg. Comp.","Equipment Related","","","","","To fabricate suitable steel bars & fix it at optimum positions on the crane for them to trigger stop at correct position.\n\nAppropriate steel bars fabricated and fitted at strategic positions on the crane. Slewing operation of the crane tried out & functional test of limit switches verified - working satisfactory.","2020-12-17","","Completed","2020-11-21","No","No","No","Internal"]
[null,null,null,null,14376,"26_29 Oct 2020 10:46:16 AM","2020-09-18","Observation","Ship Staff","Ship Staff Insp.","HPP # 4 (diesel engine) - starting battery set observed deteriorated and towards end of life.","Cargo Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","To replace by new spare.\n\n\n\nBattery set replaced by new set. After initial charging, tested by giving 3 consecutive starts - working satisfactory.","2020-12-17","AQUA200144","Completed","2020-09-30","No","No","No","Internal"]
[null,null,null,null,14377,"26_29 Oct 2020 10:53:58 AM","2020-09-18","Observation","Ship Staff","Ship Staff Insp.","IGG - Repeat flame failure","Inert Gas","Eng. / Strg. Comp.","Equipment Related","","","","","Main & pilot burner overhauled; ignitor cleaned; solenoid valves for main & pilot burner inspected/overhauled.\n\nFlame detectors checked - found one defective.\n\nDefective flame detector removed from service; unit fired - operation satisfactory.\n\nOperation in auto mode noted to be normal at 25% load setting.","2020-12-17","","Completed","2020-09-22","No","No","No","Internal"]
[null,null,null,null,14378,"26_29 Oct 2020 10:57:19 AM","2020-09-18","Observation","Ship Staff","Ship Staff Insp.","Main engine - OMD fail alarm trigger & reset by itself - repetition of alarm noted.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Unit to be cleaned.\n\n\n\nCleaning & calibration of the unit carried out - working satisfactory.","2020-09-30","","Completed","2020-09-23","No","No","No","Internal"]
[null,null,null,null,14379,"26_29 Oct 2020 11:31:44 AM","2020-09-18","Observation","Ship Staff","Ship Staff Insp.","Main Engine - Sump tank level alarm trigger at level 42 cm (normally comes around 33 cm); oil taken till 48 cm sounding but alarm still exists.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","To investigate & troubleshoot the fault.\n\n\n\nFault found at the terminal connection on top of the unit; same rectified - working satisfactory.","2020-12-17","","Completed","2020-09-24","No","No","No","Internal"]
[null,null,null,null,14380,"26_29 Oct 2020 11:36:32 AM","2020-09-18","Defect","Ship Staff","Ship Staff Insp.","Wash basin at ER toilet space - water found isolated due to basin tap not holding - no spare on board.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","Hot water line isolated; cold water line modified and arrangement made for cold water use by fitting ball valve & curved pipe at its free end.","2020-12-17","","Completed","2020-09-25","No","No","No","Internal"]
[null,null,null,null,16325,"26_21 Dec 2020 09:28:10","2020-09-18","Observation","Ship Staff","Ship Staff Insp.","Boiler feed water auto valve - leaking from gland; the gland nut threads are deteriorated and wasted thus unable to hold the tightened position.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","We carried out modification to the gland securing arrangement.\n\nThis modification provides a balanced pressure on the round gland nut (the wasted threads have been polished for smooth movement over the raised gland pocket).\n\n","2020-12-17","","Completed","2020-11-25","No","No","No","Internal"]
[null,null,null,null,16327,"26_25 Nov 2020 09:53:49","2020-09-18","Defect","Ship Staff","Ship Staff Insp.","Galley Hot Plate - 2 out of 4 not working","Accommodation,Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","Found wires broken at hot plate connection & lugs burnt.\n\nFor one hot plate, deteriorated section of wire chopped off & fitted with new lugs.\n\nFor second one, complete wire from the operating switch renewed & fitted with new lugs.","2020-12-17","","Completed","2020-10-01","No","No","No","Internal"]
[null,null,null,null,16326,"26_24 Nov 2020 21:12:26","2020-09-19","Defect","Ship Staff","Ship Staff Insp.","440VAC earth fault alarm trigger - identified to be from ER fan # 2 & 4; Both switched Off for rectification of fault.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","To investigate, troubleshoot & rectify.\n\n\n\nOn investigation found the earth fault coming from:\n\na) terminal box at the ER fan # 2 - rectified by renewing cable lugs and chopping off the deteriorated cable end.\n\n\n\nb) Junction box for fans - rectified by renewing cable lugs & choffing off the detriorated cable end. Also for one cable we had to use normal terminal strip (with plastic insulation covering) for connecting as no permanent dedicated cable strips found on board.\n\nJunction box inspected after operation & found in good condition.","2020-12-18","","Completed","2020-09-26","No","No","No","Internal"]
[null,null,null,null,16328,"26_24 Nov 2020 21:17:11","2020-09-19","Observation","Ship Staff","Ship Staff Insp.","Steam leak at Boiler top from connection for copper tubing","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","The leaky connection made good by reneweing the defective ferrule.","2020-12-18","","Completed","2020-09-29","No","No","No","Internal"]
[null,null,null,null,16329,"26_21 Dec 2020 09:21:33","2020-09-19","Observation","Ship Staff","Ship Staff Insp.","Main Engine Exhaust trunking before EGB - the protective sheathing for laagging found deteriorated.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","Deteriorated section of metal sheathing renewed","2020-12-18","","Completed","2020-12-14","No","No","No","Internal"]
[null,null,null,null,16330,"26_25 Nov 2020 10:10:57","2020-09-19","Observation","Ship Staff","Ship Staff Insp.","HFO Purifier # 1 - both pumps required to be run else low pressure alarm trigger for the purifier.","E/R - Pumps,E/R - Purifier","Eng. / Strg. Comp.","Equipment Related","","","","","Relief Valve for the feed pump overhauled & adjusted to increase the pressure but no significant improvement.\n\nSuction gauge renewed - new gauge reads only 0.2 kg/cm2 due to tank head.\n\nAttemptted in vain, to inspect & clear the suction line as the QCV at the HFO settling tank observed not holding, possibly due to deposits that are reducing the flow to the purifier feed pump.\n\nSettling tank emptied, ventilated and manually cleaned / de-mucked. QCV cleaned / overhauled  & inspected - okay.\n\nAfter inspection & securing all openings, oil taken into tank & HFO purifier # 1 run with its dedicated pump - working satisfactory.","2020-12-18","","Completed","2020-12-26","No","No","No","Internal"]
[null,null,null,null,17924,"26_19 Feb 2021 6:37:06 PM","2020-09-20","Observation","Ship Staff","Ship Staff Insp.","Sounding pipes rusty & caps seized for the following tanks:\n\n1) M.G.O. Serv. Tk\n\n2) M.D.O. Sett. Tk\n\n3) M.D.O. Serv. Tk\n\n4) LS H.F.O. Serv. Tk\n\n5) H.F.O. Serv. Tk\n\n6) H.F.O. Sett. Tk","Deck - Pipe / Fittings,Hull & Tanks","Eng. / Strg. Comp.","Equipment Related","","","","","To de-rust & free up the caps.\n\n31-Oct-2020 =de-rusted &  freed up for S.No. 1 to 3\n\n12-Nov-2020 = de-rusted & freed up for S.No. 4 & 5\n\n19-Dec-2020 = de-rusted & freed up for S.No. 6 - had to fabricate tool to apply additional force to open this cap.","2020-12-19","","Completed","2020-12-19","No","No","No","Internal"]
[null,null,null,null,16331,"26_30 Dec 2020 15:43:49","2020-09-20","Observation","Ship Staff","Ship Staff Insp.","Pipe Vise broken during use","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","To renew.\n\nNew pipe vise received & fitted - satisfactory.","2020-12-19","AQUA200149","Completed","2020-10-22","No","No","No","Internal"]
[null,null,null,null,17922,"26_19 Feb 2021 6:41:08 PM","2020-09-23","Observation","Ship Staff","Ship Staff Insp.","Waste Oil Service tank - heating coil noted to have pin hole","E/R - Pipes/ valves & fittings,Hull & Tanks","Eng. / Strg. Comp.","Equipment Related","","","","","To carry out soft patch repair.\n\nRepaired by soft patch - satisfactory.\n\nPermanent repairs to be carried out in dry dock.","2020-09-30","","Completed","2020-09-24","No","No","No","Internal"]
[null,null,null,null,14381,"26_29 Oct 2020 11:03:51 AM","2020-09-23","Critical Equipment,Defect","Ship Staff","Ship Staff Insp.","Emergency DG - during routine operational test of the hydraulic starter, unable to start the engine even after repeated attempts.\n\n\n\nSuspect accumulator has lost its Nitrogen gas to assist accumulate hydraulic energy required for engine start","Critical Equip.","Emgcy. Systems","Equipment Related","","","","","New accumulator on board but required relay valve to be reused. With all attempts made, we removed the connection of relay valve to accumulator but observed the threads are damaged.\n\nOn receipt of new relay valve, hydraulic unit assembled & tried out - satisfactory.","2020-10-22","AQUA200143\n\nAQUA205081","Completed","2020-10-04","No","No","No","Internal"]
[null,null,null,null,16332,"26_25 Nov 2020 11:12:11","2020-09-23","Observation","Ship Staff","Ship Staff Insp.","Dom Ref Plant - Filter drier cartridge not renewed for long time since 2013.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Replaced by new cartridge on board.\n\nRequisition raised for spare cartridges for future use & received at Singapore","2020-12-22","AQUA200160","Completed","2020-10-19","No","No","No","Internal"]
[null,null,null,null,17923,"26_19 Feb 2021 6:46:02 PM","2020-09-24","Observation","Ship Staff","Ship Staff Insp.","EGB Wash Drain Tank - for one section drain line broke at the tank before the isolating valve. HOT WORK at site required for permanent job","Hull & Tanks","Eng. / Strg. Comp.","Equipment Related","","","","","Broken protruding part cropped off and a blank placed & secured by cold work.\n\nPermanent repairs to be carried out in dry dock.","2020-09-30","","Completed","2020-09-24","No","No","No","Internal"]
[null,null,null,null,16333,"26_24 Nov 2020 21:29:52","2020-09-24","Observation","Ship Staff","Ship Staff Insp.","EGB wash drain line mouth found with no cover - this leads to soot falling inside of the pipe & blocking it & also cause for seizure of isolating valve.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","New cover with handle and locating sleeve fabricated and placed on the mouth.\n\nThis cover to be removed only when water washing is being carried out & then placed back in position prior closing the manhole cover.","2020-12-23","","Completed","2020-09-24","No","No","No","Internal"]
[null,null,null,null,16336,"26_24 Nov 2020 21:24:56","2020-09-24","Observation","Ship Staff","Ship Staff Insp.","EGB wash drain line isolating valve found seized.\n\nOn dismantling found totally seized in half open position.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","New gate valve fitted from onboard spare","2020-12-23","","Completed","2020-09-24","No","No","No","Internal"]
[null,null,null,null,14382,"26_28 Oct 2020 12:11:47 PM","2020-09-26","Defect","Ship Staff","Ship Staff Insp.","Steam line of COT 1 Port was leaking","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","","","","","Pipe would be removed, a new pipe would be fabricated to put in place.","2020-12-30","","Completed","2020-10-24","No","No","No","Internal"]
[null,null,null,null,16340,"26_25 Nov 2020 11:22:54","2020-09-26","Observation","Ship Staff","Ship Staff Insp.","AE # 3 - auto synchro fail & stand-by AE # 1 started and came on load.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","ACB drawn out, front cover opened – found closing coil securing screws were loose, same tightened in place. Also observed the closing lever at the push button was not retreiving by the spring force thus not resetting to the ready to operate position; same freed up & lubricated. ACB tested manually and movement visually checked – normal.\n\nACB boxed back & tried out in auto  mode – worked normal; repeated 5 times – make & break of the ACB noticed normal with no alarm trigger.\n\nAt Singapore on 19-Oct-2020, all three ACBs serviced by shore team.","2020-12-25","AQUA205087","Completed","2020-10-19","No","No","No","Internal"]
[null,null,null,null,16339,"26_30 Nov 2020 10:58:30","2020-09-28","Observation","Ship Staff","Ship Staff Insp.","Atomising steam low pressure alarm observed not functional.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","to investigate the root cause and rectify.\n\n\n\nThe pressure switch was not responding with the change in pressure.\n\nafter investigation and checks, we noted that the position of the electrical switch unit cannot be adjusted for this purpose.\n\nSo, we adjusted the position of adjustable screws at the two ends of the fulcrum to enable the switch make/break as per pressure change around the set point.\n\nArrangement tested - triggers at about 1.5 bar falling pressure and resets at 2.4 bar rising pressure. The alarm trigger trips the boiler.\n\nThe setting adjusted to trigger alarm & trip at 2.0 bar falling pressure in line with the maker's guidelines.\n\n","2020-12-27","","Completed","2020-11-27","No","No","No","Internal"]
[null,null,null,null,14383,"26_29 Oct 2020 11:15:37 AM","2020-09-30","Observation","Ship Staff","Ship Staff Insp.","Suspect deteriorated control arrangement for the \"capacity control valve.\n\nAlso noted that the potentiometer in the panel for emergency operation are deteriorated - one for capacity control valve - a touch on the lock lever itself moves the valve (lock to unlock position results in the capacity control valve moving from shut to open position & vice versa).","Inert Gas","Eng. / Strg. Comp.","Equipment Related","","","","","IGG given at 25% load with vigilant monitoring of the sea water discharge.\n\nRequisition raised for spares.\n\nService arranged for Singapore attendance.\n\n\n\nSpool valve on capacity control unit renewed.\n\nDefective flame detector renewed.\n\nAll three potentiometer renewed & tested for operation in emergency mode - working satisfactory.\n\nOperation of capacity control valve checked with both IG fans - improved response.","2020-12-29","AQUA200147\n\nAQUA205090","Completed","2020-10-21","No","No","No","Internal"]
[null,null,null,null,14384,"26_28 Oct 2020 5:18:35 PM","2020-09-30","Defect","Ship Staff","Ship Staff Insp.","Leaking air line abreast of cargo manifold","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","","","","","New pipe to be fabricated and put in place","2020-11-30","","Completed","2020-10-23","No","No","No","Internal"]
[null,null,null,null,16334,"26_30 Dec 2020 15:58:04","2020-09-30","Observation","Ship Staff","Ship Staff Insp.","Engine Room DB tanks' sounding pipe vent arrangement not fully functional.","Hull & Tanks","Eng. / Strg. Comp.","Equipment Related","","","","","Air vent arrangement overhauled & made operational - working satisfactory for all DB tanks","2020-10-29","","Completed","2020-10-14","No","No","No","Internal"]
[null,null,null,null,16335,"26_25 Nov 2020 08:25:59","2020-10-01","Observation","Ship Staff","Ship Staff Insp.","ESB - 220 VAC earth fault trigger.\n\nFault located to emergency light fitting at stbd side life raft - glass bulb detached from its securing holder.\t","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","The damaged lamp replaced. The wiring condition for the holder inspected - in good working condition.","2020-12-31","","Completed","2020-10-01","No","No","No","Internal"]
[null,null,null,null,16337,"26_30 Dec 2020 20:35:07","2020-10-02","Observation","Ship Staff","Ship Staff Insp.","LSMGO bunker manifold valve on the port aft found in open position & cannot be closed.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Same dimension wafer type valve found on board, same used to replace the defective one. The LSMGO that came out during valve removal safely collected in clean container and put back in bunker tank. The gear operating pin is damaged.","2021-01-02","","Completed","2020-12-22","No","No","No","Internal"]
[null,null,null,null,16338,"26_18 Dec 2020 2:35:23 PM","2020-10-04","Defect","Ship Staff","Ship Staff Insp.","Broken acessladder WBT 1S","Hull & Tanks","Cargo / Ballast Systems","Equipment Related","","","","","New ladder to be placed with nut and bolt arrangement with 3 coats of primer.","2021-01-30","","Completed","2020-11-07","No","No","No","Internal"]
[null,null,null,null,16341,"26_18 Dec 2020 3:01:40 PM","2020-10-06","Defect","Ship Staff","Ship Staff Insp.","WBT acess ladder for 3WGS corroded and broken .","Hull & Tanks","Cargo / Ballast Systems","Equipment Related","","","","","New ladder to be placed with nut and bolt arrangement with 3 coats of primer.","2021-01-30","","Completed","2020-12-04","No","No","No","Internal"]
[null,null,null,null,16342,"26_30 Dec 2020 16:03:26","2020-10-06","Observation","Ship Staff","Ship Staff Insp.","Hose handling crane - hoist up limit switch not activated at required hook position - noted physical position of the limit switch is farther away.","Deck - Machinery","Eng. / Strg. Comp.","Equipment Related","","","","","Limit switch operation verified by manually activating it during hoist up operation - working good.\n\nThe limit switch re-located & secured at the optimum position for it to stop further hook movement in hoist up direction.","2021-01-05","","Completed","2020-10-08","No","No","No","Internal"]
[null,null,null,null,16343,"26_18 Dec 2020 2:53:56 PM","2020-10-08","Defect","Ship Staff","Ship Staff Insp.","Damaged, corroded WBT acess laddrer for WBT 2 Stbd","Hull & Tanks","Cargo / Ballast Systems","Equipment Related","","","","","New ladder to be placed with nut and bolt arrangement with 3 coats of primer.","2021-01-30","","Completed","2020-11-25","No","No","No","Internal"]
[null,null,null,null,14385,"26_28 Oct 2020 5:21:12 PM","2020-10-10","Defect","Ship Staff","Ship Staff Insp.","FW line to deck eyewash station leaking","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","","","","","Old pipe to be taken out and new pipe to be fabricated for same","2020-12-15","","Completed","2020-10-29","No","No","No","Internal"]
[null,null,null,null,16344,"26_30 Dec 2020 16:18:44","2020-10-10","Observation","Ship Staff","Ship Staff Insp.","AE # 1 ACB - securing bolts sheared off while opening for routine maintenance checks.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","Broken bolt drilled & extracted.\n\nNew appropriate bolt used to secure the ACB - working good.","2020-10-11","","Completed","2020-10-10","No","No","No","Internal"]
[null,null,null,null,16345,"26_30 Dec 2020 16:21:43","2020-10-12","Observation","Ship Staff","Ship Staff Insp.","Ejector pump discharge pipe found leaking","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Leaky pipe section removed.\n\nNew pipe fabricated in engine room workshop & fitted in place.","2020-10-15","","Completed","2020-10-12","No","No","No","Internal"]
[null,null,null,null,17925,"26_19 Feb 2021 6:50:14 PM","2020-10-15","Observation","Ship Staff","Ship Staff Insp.","Fire Detection System - sensor & base deteriorated and non-operational for position 101 in engine room above main engine.","LSA / FFA","Eng. / Strg. Comp.","Equipment Related","","","","","Defective sensor isolated. Requisition raised.\n\nRenewed the flame detector together with its base using new supply and the detector address changed to 101 from its default setting.","2021-01-14","AQUA200172","Completed","2021-01-05","No","No","No","Internal"]
[null,null,null,null,16346,"26_30 Dec 2020 16:24:47","2020-10-15","Observation","Ship Staff","Ship Staff Insp.","LSFO service tank condensate return line isolating vlave found not holding","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Valve replaced by spare one on board.","2021-01-14","","Completed","2020-10-25","No","No","No","Internal"]
[null,null,null,null,17927,"26_19 Feb 2021 6:53:29 PM","2020-10-16","Observation","Ship Staff","Ship Staff Insp.","Aux boiler - pressure gauge pipe observed leaking.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","Leakage rectified - connection joint renewed.","2020-10-17","","Completed","2020-10-16","No","No","No","Internal"]
[null,null,null,null,17926,"26_19 Feb 2021 6:55:33 PM","2020-10-17","Observation","Ship Staff","Ship Staff Insp.","IGG SW inlet pressure gauge observed incorrect display.","Inert Gas","Eng. / Strg. Comp.","Equipment Related","","","","","Defective pressure gauge renewed","2020-10-20","","Completed","2020-10-17","No","No","No","Internal"]
[null,null,null,null,14370,"26_28 Oct 2020 5:28:10 PM","2020-10-19","Other","Ship Staff","Ship Staff Insp.","Conduit line on uppder deck at break of accommodation corroded.","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","Equipment Related","","","","","Thorough surface preparation with covering of conduit line with painting and stenciling","2020-12-15","","Completed","2020-04-11","No","No","No","Internal"]
[null,null,null,null,14371,"26_28 Oct 2020 8:19:34 PM","2020-10-20","Observation","Ship Staff","Ship Staff Insp.","HPP# 3 (diesel engine) - starter battery pack reached end of life - engine not starting & battery voltage dips to about 10 V","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","To Procure new battery set.\n\n\n\nNew lifeboat battery set used to start the engine.\n\n\n\n\n\n\n\nNew received battery set have round terminals - need to modify the onboard small size terminal lugs to cater to existing bolt/nut connection.\n\n\n\nLugs modified and fitted; battery set charged & put in use - tested by giving 3 consecutive starts - working satisfactory","2020-12-19","AQUA205093","Completed","2020-10-29","No","No","No","Internal","BATTERIES RENEWED."]
[null,null,null,null,16691,"26_5 Jan 2021 10:37:53 AM","2020-10-20","Observation","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","WBT 1 Port nad 1 Stbd sighted from deck level setion of vertical ladder thinned more then 50 %","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","2.16","Medium","","","NEw ladder fitted in WBT 1 Port and 1 Stbd","2020-11-15","","Completed","2020-10-29","No","No","No","External"]
[null,null,null,null,16692,"26_5 Jan 2021 10:52:55 AM","2020-10-20","Observation","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","When attending mooring manual brakes port side aft mooring winch , vessel crew has to stand in between two taut mooring ropes passing at a distance of 0.5 mtr","Deck - Mooring Machinery","Mooring","Equipment Related","9.8","Medium","","","Ship staff well aware with rope tightening procedures, in addition  stencile for caution when handling brake has been marked near the winches","2020-11-15","","Completed","2020-10-25","No","No","No","External"]
[null,null,null,null,16693,"26_5 Jan 2021 11:11:35 AM","2020-10-20","Observation","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","1. Electric cable conduit pipes at the poop were found to be heavily corroded .                2. Fresh water supply line to the eye wash/contamination station near centre secrion aft leaking.                                          3. Most of cargo heating lines found corroded , at some section flakes of rust scales were apparent.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","11.4","Very High","","","1. Conduit lines on main deck below boat deck repaired, photos for same sent                               2. Fresh water line gasket for leaking fresh water line changed and tested for integrity                        3. Special compound based heaing coil provided to vessel to be applied on heating coil","2020-11-15","","Completed","2020-10-31","No","No","No","External"]
[null,null,null,null,16694,"26_5 Jan 2021 10:44:35 AM","2020-10-20","Observation","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","MBL was 67 T, the morring line fitted to the after spring (7 & 8) and stern line (11 & 12) LDBF was 60.3 T 100-105% of the ship design MBL","Deck - Mooring Machinery","Mooring","Inappropriate Procedure","9.7","Medium","","",".Prior departure Singapore corrected certificate received, circular pased in fleet to check all certificates when received.","2020-11-15","","Completed","2020-10-21","No","No","No","External"]
[null,null,null,null,16347,"26_21 Dec 2020 09:32:44","2020-10-20","Observation","Ship Staff","Ship Staff Insp.","Sewage Treatment Plant vent pipe - several sections found deteriorated & wasted.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Deteriorated sections renewed","2021-01-19","","Completed","2020-11-03","No","No","No","Internal"]
[null,null,null,null,16348,"26_21 Dec 2020 09:36:38","2020-10-20","Observation","Ship Staff","Ship Staff Insp.","Suction pipe from No.2 H.F.O. Tank (S) - observed lagging is black with old oil","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Renewed oil soaked lagging","2021-01-19","","Completed","2020-11-06","No","No","No","Internal"]
[null,null,null,null,16349,"26_30 Dec 2020 17:16:27","2020-10-20","Observation","Ship Staff","Ship Staff Insp.","440 VAC low insulation alarm trigger at each hoist operation for provision crane","Deck - Machinery","Eng. / Strg. Comp.","Equipment Related","","","","","440VAC earth triggerred at each hoist/lower operation of the hook.\n\nFound the terminal strip in the junction box inside the crane column is giving earth fault. Terminal strip replaced by spare on board; the connection lugs renewed & crane tested for operation - working good.","2020-12-19","","Completed","2020-11-29","No","No","No","Internal"]
[null,null,null,null,16350,"26_30 Dec 2020 17:29:57","2020-10-20","Observation","Ship Staff","Ship Staff Insp.","Incinerator - secondary blower drawing high current.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Secondary blower overhauled, damged impeller renewed; motor renewed, nozzle renewed. Electric cable inside was laid close to the impeller, same re-routed to keep it away from the impeller.","2020-11-19","AQUA200138","Completed","2020-10-20","No","No","No","Internal"]
[null,null,null,null,16351,"26_30 Dec 2020 18:33:52","2020-10-20","Observation","Ship Staff","Ship Staff Insp.","Incinerator not starting on overhaul of primary & secondary burners.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Fault traced to voltage drop due to earth fault in the emergency stop circuit, same rectified.","2020-11-20","","Completed","2020-10-21","No","No","No","Internal"]
[null,null,null,null,16352,"26_30 Dec 2020 20:46:34","2020-10-20","Observation","Ship Staff","Ship Staff Insp.","ESB - 220 VAC low insulation alarm trigger","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","Fault traced to light fixture in Emer DG room.\n\nFault rectified by renewing the deteriorated cables - Okay ","2020-10-22","","Completed","2020-10-20","No","No","No","Internal"]
[null,null,null,null,16353,"26_30 Dec 2020 17:34:20","2020-10-21","Observation","Ship Staff","Ship Staff Insp.","Incinerator - secondary burner flame eye sensor not working.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Found the cable for the secondary burner flame eye having earth fault.\n\nDefective cable renewed - working good.","2020-11-20","","Completed","2020-10-21","No","No","No","Internal"]
[null,null,null,null,16354,"26_30 Nov 2020 11:04:43","2020-10-22","Observation","Ship Staff","Ship Staff Insp.","I in number hot plate reported not working.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","On inspection found that the cable lugs had burnt out; same renewed.","2021-01-21","","Completed","2020-10-31","No","No","No","Internal"]
[null,null,null,null,16355,"26_30 Dec 2020 18:54:19","2020-10-23","Observation","Ship Staff","Ship Staff Insp.","Main Engine - Unit # 4 indicator cock observed leaking","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Defective indicator cock replaced by spare one; annealed copper washers used in assembly","2020-10-24","","Completed","2020-10-23","No","No","No","Internal"]
[null,null,null,null,17928,"26_19 Feb 2021 7:00:26 PM","2020-10-26","Observation","Ship Staff","Ship Staff Insp.","General Service Air system - 30k7 pressure reducing valve unable to cope up for additional demand.\n\nValve opened & found no diaphragm & spring; it had been modified for fixed air quantity delivery using long screw holding valve disc in position.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Requisition raised for spares\n\nDefective pressure reducing valve replaced by overhauled valve removed from control air system - Working satisfactory","2021-04-25","AQUA200182","Completed","2021-02-13","No","No","No","Internal"]
[null,null,null,null,14475,"26_2020-11-06 9:05:26 AM","2020-10-26","Defect","Ship Staff","Ship Staff Insp.","Eye wash line on deck corroded break of accomodation","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","","","","","New pipe to be fabricated and put back in place, with painting.","2020-11-30","","Completed","2020-09-11","No","No","No","Internal","Noted."]
[null,null,null,null,17929,"26_19 Feb 2021 7:02:46 PM","2020-10-28","Observation","Ship Staff","Ship Staff Insp.","Control Air System - 30k7 pressure reducing valve performance deteriorated.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Requisition raised.\n\nReplaced by newly received complete valve - working satisfactory.","2021-04-27","AQUA200182","Completed","2021-01-28","No","No","No","Internal"]
[null,null,null,null,14372,"26_2020-11-01 6:57:04 PM","2020-10-28","Defect","Ship Staff","Ship Staff Insp.","Port bunker vent cover plates corroded.","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","External Factors","","","","","New cover plates to be made and replaced","2020-12-30","","Completed","2020-11-13","No","No","No","Internal","Noted."]
[null,null,null,null,14478,"26_2020-11-06 9:08:10 AM","2020-10-29","Defect","Ship Staff","Ship Staff Insp.","Bunker vent pipe break of accomodation port side holed when chipping","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","","","","","same to repaired painted and stensiled","2020-12-31","","Completed","2020-12-11","No","No","No","Internal","Please send repair plan to us for review!"]
[null,null,null,null,16356,"26_30 Dec 2020 20:39:44","2020-10-29","Observation","Ship Staff","Ship Staff Insp.","ESB - 220 VAC earth fault trigger","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","Fault traced to light fixture in Steering gear room - same rectified by renewing the deteriorated cables in the light fixture.","2020-10-31","","Completed","2020-10-29","No","No","No","Internal"]
[null,null,null,null,14474,"26_2020-11-06 9:13:34 AM","2020-10-30","Defect","Ship Staff","Ship Staff Insp.","Waste oil tank vent pipe poop deck next to CO2 room badly carroded , with supports worn out","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","","","","","New support to be fabricated. and damaged vent pipe to be repaired.","2020-12-31","","Completed","2020-10-11","No","No","No","Internal","Noted action proposed. Also suggest to apply proper paint coats for corrosion protection."]
[null,null,null,null,16357,"26_30 Nov 2020 11:24:39","2020-10-30","Observation","Ship Staff","Ship Staff Insp.","Fuel lever in ECR - fine control knob was observed to be seized and inoperable","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","The unit removed, cleaned thoroughly and lubricated. The movement checked for operation - found smooth operation.\n\nThe fine control unit fitted in place and operation verified - in good working condition.","2021-01-29","","Completed","2020-11-01","No","No","No","Internal"]
[null,null,null,null,16358,"26_30 Dec 2020 20:50:07","2020-10-30","Observation","Ship Staff","Ship Staff Insp.","Bilge pump discharge pressure gauge observed leaking","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Defective pressure gauge replaced by new spare one.","2020-12-29","","Completed","2020-10-30","No","No","No","Internal"]
[null,null,null,null,14476,"26_2020-11-06 9:18:15 AM","2020-10-31","Breakdown","Ship Staff","Ship Staff Insp.","Cabin of third offier faulty faucet","Accommodation","Crew Management","Equipment Related","","","","","New faucet to be put in palce","2020-11-30","","Completed","2020-02-11","No","No","No","Internal","Noted."]
[null,null,null,null,14477,"26_2020-11-06 9:21:07 AM","2020-10-31","Defect","Ship Staff","Ship Staff Insp.","Third engineer cabin faulty shower head","Accommodation","Crew Management","Equipment Related","","","","","New shower head to be put in place.","2020-11-30","","Completed","2020-02-11","No","No","No","Internal","Noted."]
[null,null,null,null,17930,"26_19 Feb 2021 7:05:30 PM","2020-11-02","Observation","Ship Staff","Ship Staff Insp.","No. 2 H.F.O. Tk (S) - found vent head in deteriorated condition","Deck - Pipe / Fittings,Hull & Tanks","Eng. / Strg. Comp.","Equipment Related","","","","","Wasted top & side covers fabricated new and fitted - satisfactory","2020-11-08","","Completed","2020-11-03","No","No","No","Internal"]
[null,null,null,null,14949,"26_16-Nov-20 5:25:55 PM","2020-11-02","Non Conformity","Owner / Marine / Tech. Suptd.","ISM Audit","Defective Cofferdam Air pipe vent.","Deck - Machinery","Crew Management","Equipment Related","1.12","Low","","","To fabricate new plates.for vent.","2020-12-30","","Completed","2020-11-26","No","No","No","Internal","Job was in progress and as per weekly report, it is completed. Please record it accirdingly."]
[null,null,null,null,16366,"26_18 Dec 2020 17:44:45","2020-11-02","Observation","Ship Staff","Ship Staff Insp.","No. 1 H.F.O.T. Tank (S) vent head found deteriorated","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Wasted top & side covers fabricated new & fitted","2021-02-01","","Completed","2020-11-03","No","No","No","Internal"]
[null,null,null,null,17931,"26_19 Feb 2021 7:09:40 PM","2020-11-03","Observation","Ship Staff","Ship Staff Insp.","Main Engine Fuel inlet main line QCV observed deteriorated due to vibration; manual control is now not operational","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Requisition raised.\n\nComplete valve replaced by newly supplied QCV - satisfactory","2021-02-02","AQUA200185","Completed","2021-01-25","No","No","No","Internal"]
[null,null,null,null,17932,"26_19 Feb 2021 7:13:38 PM","2020-11-04","Observation","Ship Staff","Ship Staff Insp.","UV Sterilizer for drinking water - observed water leak due to cracked quartz. no spare on board.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","Requisition raised.\n\nDamaged parts replaced by newly received spares - quartz, lamp & lamp holder.","2021-02-03","AQUA200186","Completed","2021-01-03","No","No","No","Internal"]
[null,null,null,null,16359,"26_18 Dec 2020 16:11:05","2020-11-04","Observation","Ship Staff","Ship Staff Insp.","Dom ref compressor # 2 - observed leak from mechanical seal in excess of guidelines by makers.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Mechanical Seal & cover renewed.\n\nCompressor sump oil drained, cleaned and new oil taken.\n\nVacuum created to remove all air that ingressed the compressor prior to putting compressor in use.","2021-02-03","","Completed","2020-11-06","No","No","No","Internal"]
[null,null,null,null,16360,"26_18 Dec 2020 16:56:49","2020-11-05","Observation","Ship Staff","Ship Staff Insp.","MGO Tank (S) Vent head observed in deteriorated condition","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Wasted top & side covers fabricated new & fitted","2021-02-04","","Completed","2020-11-06","No","No","No","Internal"]
[null,null,null,null,16361,"26_18 Dec 2020 17:22:26","2020-11-05","Observation","Ship Staff","Ship Staff Insp.","Waste Oil Service tank vent head found in deteriorated condition","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Wasted top & side covers fabricated new & fitted","2021-02-04","","Completed","2020-11-06","No","No","No","Internal"]
[null,null,null,null,16362,"26_18 Dec 2020 17:29:41","2020-11-05","Observation","Ship Staff","Ship Staff Insp.","Sewage Treatment Plant vent head found in deteriorated condition","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Wasted top & side covers fabricated new & fitted","2021-02-04","","Completed","2020-11-06","No","No","No","Internal"]
[null,null,null,null,17933,"26_19 Feb 2021 7:18:07 PM","2020-11-06","Observation","Ship Staff","Ship Staff Insp.","Lube Oil Purifier # 2 - not in use for long.\n\nOn opening for pre-operation inspection, found several parts damaged.","E/R - Purifier","Eng. / Strg. Comp.","Equipment Related","","","","","Requisition raised.\n\nPurifier assembled using newly received spares. & tried out - satisfactory.","2021-05-05","AQUA200190","Completed","2021-02-08","No","No","No","Internal"]
[null,null,null,null,16363,"26_30 Nov 2020 11:29:54","2020-11-06","Observation","Ship Staff","Ship Staff Insp.","Air leak at the flange of cleaning water pipe on main engine air cooler.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","The deteriorated gasket renewed - in good working condition","2021-02-05","","Completed","2020-11-07","No","No","No","Internal"]
[null,null,null,null,16364,"26_30 Nov 2020 12:50:07","2020-11-06","Observation","Ship Staff","Ship Staff Insp.","ME unit # 3 - indicator cock observed leaking at sealing surface","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Leaky Gasket renewed.","2020-11-20","","Completed","2020-11-07","No","No","No","Internal"]
[null,null,null,null,16365,"26_18 Dec 2020 16:14:48","2020-11-06","Observation","Ship Staff","Ship Staff Insp.","FWG - feed regulating valve observed leaking.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Feed regulating valve overhauled.\n\nObserved diaphragm previously used from gasket material which broke resulting in leak. Another gasket cut to size & fitted.","2021-02-05","","Completed","2020-11-10","No","No","No","Internal"]
[null,null,null,null,16321,"26_18 Dec 2020 16:05:53","2020-11-08","Observation","Ship Staff","Ship Staff Insp.","Discharge valve not holding for boiler feed water pump # 1 - found damaged; no spare on board","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Requisition raised.\n\nDelivery valve renewed using new supply valve.","2021-02-07","AQUA200191","Completed","2021-02-04","No","No","No","Internal","Job is reported completed during weekly work done reporting. Please update completion."]
[null,null,null,null,16367,"26_5 Dec 2020 07:38:25","2020-11-08","Observation","Ship Staff","Ship Staff Insp.","Aux Boiler Feed water pump # 1 observed leaking at mechanical seal.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","","","","","Pump overhauled; DE mechanical seal, NDE sleeve, both end bearings set renewed. NDE mechanical seal has been replaced by another old one in better condition.\n\nImpellers had rubbing marks due to NDE bearing damage.","2021-02-07","","Completed","2020-11-11","No","No","No","Internal"]
[null,null,null,null,16368,"26_5 Dec 2020 07:42:27","2020-11-08","Observation","Ship Staff","Ship Staff Insp.","Aux Boiler Feed water pump # 1 - Observed high ampere drawn during operation.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","Motor overhauled and both bearings renewed.\n\nPump overhauled.\n\nPump & motor alignment carried out.","2021-02-07","","Completed","2020-11-11","No","No","No","Internal"]
[null,null,null,null,14950,"26_2020-11-15 7:41:36 AM","2020-11-10","Other","Ship Staff","Ship Staff Insp.","Book shelf not secured , danger in case of  rolling","Accommodation","General Appearance","Behaviour Based","","","","","New securing bars to be put in place.","2020-11-30","","Completed","2020-11-25","No","No","No","Internal","Job is completed as per weekly work done report. Please record here completion date."]
[null,null,null,null,17934,"26_19 Feb 2021 7:21:31 PM","2020-11-12","Observation","Ship Staff","Ship Staff Insp.","ME Scavenge Box Drain Tank outlet valve found malfunctioning.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Upon dismantling found the operating spindle is broken. Spindle from another valve used & fitted - satisfactory.","2020-11-18","","Completed","2021-11-12","No","No","No","Internal"]
[null,null,null,null,14951,"26_22 Nov 2020 5:08:06 PM","2020-11-15","Other","Ship Staff","Ship Staff Insp.","Steam return line damged spool piece near COT 1 stbd","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","","","","","New spool piece to be fabricated","2020-12-29","","Completed","2020-12-05","No","No","No","Internal","New Spool piece was already fabricated and replaced. Please record job as completed."]
[null,null,null,null,17935,"26_19 Feb 2021 9:39:30 PM","2020-11-16","Observation","Ship Staff","Ship Staff Insp.","Main Engine unit # 1 - top piston ring found broken at S=Lock. Piston ring intact and moving.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Under observation till suitable opportunity for unit overhaul.\n\nUnit overhaul carried out, spare overhauled piston with new piston rings used together with overhauled stuffing box. - satisfactory","2021-02-15","","Completed","2020-11-29","No","No","No","Internal"]
[null,null,null,null,17936,"26_19 Feb 2021 9:46:44 PM","2020-11-18","Observation","Ship Staff","Ship Staff Insp.","Boiler water feed pump # 3 - observed valves not holding","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Both suction & delivery lines blanked to stop water leak filling up engine room.\n\nRequisition raised.\n\nBoth suction & delivery valves renewed using new supply.","2021-02-17","AQUA200191","Completed","2021-02-04","No","No","No","Internal"]
[null,null,null,null,17912,"26_19 Feb 2021 9:42:27 PM","2020-11-18","Observation","Ship Staff","Ship Staff Insp.","Boiler water feed pump # 3 observed leaking from mechanical seals - no spare mechanical seal on board.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","","","","","Requisition raised.\n\nPump overhauled using new spares & tried out - satisfactory.","2021-05-17","AQUA200184","Completed","2021-03-30","No","No","No","Internal","Spares connected, carry out overhaul and revert completion/closure."]
[null,null,null,null,17937,"26_19 Feb 2021 9:51:36 PM","2020-11-21","Observation","Ship Staff","Ship Staff Insp.","Aux boiler feed water valves at the boiler for auto feed line observed not holding when shut.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","Requisition raised for new valves.\n\nDefective valves replaced by new supply valves.","2021-02-20","AQUA200191","Completed","2021-01-25","No","No","No","Internal"]
[null,null,null,null,17938,"26_19 Feb 2021 10:01:01 PM","2020-11-21","Observation","Ship Staff","Ship Staff Insp.","Aux boiler - feed water valves at boiler for manual feed line observed not holding when shut. No spare valves on board","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","Requisition raised.\n\nAngle valve replaced by overhauled valve removed from auto feed line.\n\nSDNR globe valve overhauled - working satisfactory. ","2021-02-20","AQUA200191","Completed","2021-02-04","No","No","No","Internal"]
[null,null,null,null,17939,"26_26 Feb 2021 1:36:59 AM","2020-11-21","Observation","Ship Staff","Ship Staff Insp.","Accommodation AC Compressor # 2 - observed oil leak off from mechanical seal is more than the maker recommendation.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","No spare mechanical seal on board. Requisition raised.\n\nMechanical seal & cover renewed using new supply spares. Compressor oil renewed. Vacuum created to extract the possible air ingressed prior putting system in use.\n\nV-belts & dryer set renewed at the same time.\n\nCompressor put in use - working satisfactory as per maker's guidelines.","2021-02-20","AQUA200192","Completed","2021-02-18","No","No","No","Internal"]
[null,null,null,null,14948,"26_22 Nov 2020 5:11:01 PM","2020-11-22","Other","Ship Staff","Ship Staff Insp.","Steam inlet pipe and return line steam trap leaking  COT 2P  .","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","","","","","New pipe to be fixed and steam trap to be changed.","2020-12-30","","Completed","2020-12-19","No","No","No","Internal","Required Pipeline material, new steam traps and valves are being ordered as per raised requisition and will be supplied, please complete relevant repairs in due course."]
[null,null,null,null,17940,"26_19 Feb 2021 10:06:02 PM","2020-11-25","Observation","Ship Staff","Ship Staff Insp.","Upper deck outside accommodation - water noticed inside FL light fixtures.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","Defective glass renewed","2020-11-30","","Completed","2020-11-25","No","No","No","Internal"]
[null,null,null,null,16369,"26_18 Dec 2020 2:24:09 PM","2020-11-26","Defect","Ship Staff","Ship Staff Insp.","Broken ballast tank access ladders for WBT 1 PORT ","Hull & Tanks","Cargo / Ballast Systems","Equipment Related","","","","","New ladder to placed with nut and bolt arrangement , ladder to be well coated with 3 coats of primer.","2021-01-30","","Completed","2020-11-30","No","No","No","Internal"]
[null,null,null,null,17941,"26_19 Feb 2021 10:12:49 PM","2020-11-27","Observation","Ship Staff","Ship Staff Insp.","in engine room, smoke detector B139 - observed plastic body broke and fell down due to end of life failure.","LSA / FFA","Eng. / Strg. Comp.","Equipment Related","","","","","Remaining base removed - it came in pieces.\n\nBroken plastic body renewed & same sensing element used & tested for operation - working satisfactory.","2020-11-29","","Completed","2020-11-27","No","No","No","Internal"]
[null,null,null,null,17942,"26_19 Feb 2021 10:15:37 PM","2020-11-28","Observation","Ship Staff","Ship Staff Insp.","Main engine unit # 6 - observed air leak at the pipe flange for start air valve.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Damaged gasket renewed - satisfactory.","2020-11-30","","Completed","2020-11-29","No","No","No","Internal"]
[null,null,null,null,17943,"26_19 Feb 2021 10:33:13 PM","2020-11-28","Observation","Ship Staff","Ship Staff Insp.","Dom Ref Compressor # 2 - tripped on overload & contactor found burnt","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","Renewed burnt contactor; on close monitoring found chattering operation of contactor.\n\nFurther investigation revealed relay malfunction was the cause.\n\nDefective relay renewed - compressor working normal.","2021-02-27","","Completed","2020-11-28","No","No","No","Internal"]
[null,null,null,null,17944,"26_19 Feb 2021 10:39:37 PM","2020-12-01","Observation","Ship Staff","Ship Staff Insp.","Aux boiler - stbd side gauge glass started leaking, same isolated for overhaul.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","To overhaul leaky gauge glass.\n\nGauge glass overhauled, deteriorated gaskets renewed & tightened as per procedure.","2020-12-15","","Completed","2020-12-05","No","No","No","Internal"]
[null,null,null,null,17945,"26_19 Feb 2021 10:43:22 PM","2020-12-02","Observation","Ship Staff","Ship Staff Insp.","Main fire pump # 2 discharge line noted leaks on two sections.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Temporary repair done to enable immediate pump use for de-ballasting operation.\n\nPipe sections removed to ER workshop & deteriorated sections repaired by welding suitable inserts.","2020-12-31","","Completed","2020-12-10","No","No","No","Internal"]
[null,null,null,null,16370,"26_18 Dec 2020 2:03:03 PM","2020-12-03","Defect","Ship Staff","Ship Staff Insp.","FW pipe line main deck near COT 5Stbd leaking","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","","","","","New FW line to be fabricated","2021-01-30","","Completed","2020-12-28","No","No","No","Internal"]
[null,null,null,null,17946,"26_19 Feb 2021 10:47:08 PM","2020-12-04","Observation","Ship Staff","Ship Staff Insp.","Sewage treatment plant - vaccumerator unit # 1 fould leak at the body.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","Vaccumerator dismatled to find end flange badly corroded & eroded.\n\nNo spare on board. Requisition raised.\n\nEnd flange reconditioned by welding & machining.\n\nVaccumerator assembled and run - working satisfactory.","2021-06-03","AQUA200209","Completed","2020-12-07","No","No","No","Internal"]
[null,null,null,null,17954,"26_19 Feb 2021 10:58:41 PM","2020-12-04","Observation","Ship Staff","Ship Staff Insp.","HFO service tank - manhole door found with tell sign of oil leak from gasket.","Hull & Tanks","Eng. / Strg. Comp.","Equipment Related","","","","","To transfer tank contents & renew gasket.\n\nTank contents transferred & deteriorated gasket for manhole door renewed. Cover cleaned & painted - satisfactory.","2020-12-31","","Completed","2020-12-07","No","No","No","Internal"]
[null,null,null,null,17947,"26_19 Feb 2021 11:09:35 PM","2020-12-07","Observation","Ship Staff","Ship Staff Insp.","Aux boiler feed water auto feed control valve performance observed deteriorated.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","To investigate & rectify.\n\nFound diaphragm damaged / broken; same renewed.","2020-12-14","","Completed","2020-12-08","No","No","No","Internal"]
[null,null,null,null,17948,"26_19 Feb 2021 11:13:18 PM","2020-12-07","Observation","Ship Staff","Ship Staff Insp.","Aux boiler fuel oil auto control valves observed leaking. No spare overhauled kit on board.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","Requisition raised.\n\nLeak rectified by fabricating teflon bush for spindle and using it with high temperature o-rings at the spindle.","2021-03-06","AQUA200207","Completed","2021-01-25","No","No","No","Internal"]
[null,null,null,null,17949,"26_19 Feb 2021 11:26:13 PM","2020-12-07","Observation","Ship Staff","Ship Staff Insp.","Boiler chemical dosing pump observed with leaks on discharge connected - noted damaged fitting was in place with soft patch repair. No spare kit on board.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","Requisition raised.\n\nDamaged parts renewed using new supply spares kit - satisfactory.","2021-03-05","AQUA200208","Completed","2021-01-05","No","No","No","Internal"]
[null,null,null,null,16371,"26_18 Dec 2020 2:13:50 PM","2020-12-07","Defect","Ship Staff","Ship Staff Insp.","Leaking FW line of galley","Accommodation","Cargo / Ballast Systems","Equipment Related","","","","","New connecting ferrul to be placed .","2021-01-30","","Completed","2020-12-13","No","No","No","Internal"]
[null,null,null,null,17950,"26_19 Feb 2021 11:34:16 PM","2020-12-09","Observation","Ship Staff","Ship Staff Insp.","Lube oil purifier motor # 1 - during overhauling observed deteriorated insulation condition of wires from stator windings to motor terminal.\n\nNo spare motor on board.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","Terminal removed, cables carfully pulled down, brittle insulation restored by applying insulation tape & sleeve. another protective sleeve placed over the arrangement.\n\nMotor dimensions have been sent to office as part of owners' motor procurement program initiated by office.","2020-12-15","","Completed","2020-12-09","No","No","No","Internal"]
[null,null,null,null,17951,"26_19 Feb 2021 11:40:08 PM","2020-12-09","Observation","Ship Staff","Ship Staff Insp.","440 VAC earth fault trigger from galley hot plates. Hot plates kept powered ON even when not in use. Idle heat not utilized causes overheating & eventual break of cable.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","Defective cables renewed.\n\nChief cook asked to switch OFF hot plates when not in use and should not be ON in idle condition.","2020-12-12","","Completed","2020-12-09","No","No","No","Internal"]
[null,null,null,null,17952,"26_19 Feb 2021 11:46:18 PM","2020-12-09","Observation","Ship Staff","Ship Staff Insp.","Dom ref plant - compressor # 2 - starter malfunction (chattering of contactor) noted at the time of auto cut off or HP trip.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","Compressor # 1 put in use.\n\ninspected starting contactor, aux block & overload relay - found that the stuck contact on aux block resulting in malfunction.\n\nRequisition raised.\n\nStarting contactor, aux block & overload relay renewed using new supply spares - working satisfactory.","2021-03-08","AQUA200213","Completed","2021-01-08","No","No","No","Internal"]
[null,null,null,null,17953,"26_19 Feb 2021 11:48:25 PM","2020-12-10","Observation","Ship Staff","Ship Staff Insp.","Cascade tank overflow line found corroded & wasted.","Hull & Tanks","Eng. / Strg. Comp.","Equipment Related","","","","","To repair/renew.\n\nCorroded section renewed - satisfactory.","2021-03-09","","Completed","2020-12-14","No","No","No","Internal"]
[null,null,null,null,17955,"26_20 Feb 2021 12:01:33 AM","2020-12-14","Observation","Ship Staff","Ship Staff Insp.","Galley hot plates not working again due to wires burnt. Found cables burnt, insulation burnt.\n\nHot plates are kept ON even when there is no cooking in progress.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","Burnt cables renewed.\n\nChief cook has be re-enforced on the fact that hot plates have to be put OFF immediately on completion of cooking. Only keep hot plates in use in ON condition.\n\nAdditionally, chief cook has been asked to keep pot of water over the hot plate for the short interim period between dishes.\n\nCaptain advised on the above situation & that monitoring has to be done for compliance else we will always be with fewer hot plates in use.","2020-12-20","","Completed","2020-12-16","No","No","No","Internal"]
[null,null,null,null,17956,"26_20 Feb 2021 12:05:17 AM","2020-12-14","Observation","Ship Staff","Ship Staff Insp.","Main engine unit # 6 - noted small oil leak at aft fuel valve on to the cylinder head.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Regular cleaning of the leaked oil done until suitable opportunity to undertake rectification.\n\nBoth fuel valves replaced by overhauled ones & main engine tried out from ECR & wheel house - satisfactory.","2020-12-31","","Completed","2020-12-18","No","No","No","Internal"]
[null,null,null,null,17957,"26_20 Feb 2021 12:13:59 AM","2020-12-15","Observation","Ship Staff","Ship Staff Insp.","Dom ref compressor # 1 noted with leak at seal more than the maker guidelines.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","to renew the seal, carry out vacuum of compressor to expel air, renew oil.\n\nRenewed mechanical seal complete. Compressor oil renewed. Vacuum created to extract possible air ingressed prior to putting system in use. System operation noted normal - satisfactory.","2021-03-14","","Completed","2020-12-17","No","No","No","Internal"]
[null,null,null,null,17958,"26_20 Feb 2021 12:17:48 AM","2020-12-15","Observation","Ship Staff","Ship Staff Insp.","FWG ejector pump suction & discharge pipes - various sections noted with leaks due to wasted pipe internals.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","to renew the wasted sections\n\nAll leaky sections in suction & discharge lines removed & shifted to ER workshop.\n\nWasted sections renewed & fitted back - satisfactory.","2021-01-31","","Completed","2021-01-20","No","No","No","Internal"]
[null,null,null,null,17959,"26_20 Feb 2021 12:21:48 AM","2020-12-16","Observation","Ship Staff","Ship Staff Insp.","Main engine unit # 6 - during under piston inspection noted oil leak from fwd fuel valve as evident from the tell signs on the piston top","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","To replace fuel valve with overhauled ones.\n\nBoth fuel valves replaced by overhauled ones in good condition & main engine tried out from ECR & wheel house - satisfactory.","2020-12-31","","Completed","2020-12-18","No","No","No","Internal"]
[null,null,null,null,17960,"26_20 Feb 2021 1:02:57 AM","2020-12-17","Observation","Ship Staff","Ship Staff Insp.","Whistle operating push button unit on stbd bridge wing broken while operating.","Navigation - Others","Navigation","Equipment Related","","","","","Power supply switched off to stop non-stop operation of whistle.\n\nSame make/model switch not available. Hence replaced by another push button switch to keep system operational.\n\nThe operation of new arrangement tested - working satsfactory.","2020-12-18","","Completed","2020-12-17","No","No","No","Internal"]
[null,null,null,null,17961,"26_20 Feb 2021 1:08:22 AM","2020-12-17","Observation","Ship Staff","Ship Staff Insp.","Cold rooms - fish room false ceiling metal sheathing found detached and bulging down.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","Appropriate steel supports fabricated from normal steel material on board. Coats of paint applied to internal & external surfaces of the fabricated arrangement prior to fitting in place.\n\nArrangement secured with the false bulkhead using clamps & screws - satisfactory.","2020-12-31","","Completed","2020-12-21","No","No","No","Internal"]
[null,null,null,null,17962,"26_20 Feb 2021 1:12:11 AM","2020-12-18","Observation","Ship Staff","Ship Staff Insp.","Emergency switchboard - 220 VAC earth fault trigger.\n\nOn troubleshooting found stbd lifeboat light faulty.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","Sleeve placed over the deteriorted cable.","2020-12-31","","Completed","2020-12-29","No","No","No","Internal"]
[null,null,null,null,17963,"26_20 Feb 2021 1:20:08 AM","2020-12-18","Observation","Ship Staff","Ship Staff Insp.","Lube oil purifier # 2 motor - during overhauling observed deteriorated insulation of wires from stator windings to the motor terminal box.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","Terminal removed, cables carefully pulled down.\n\ninsulation restored by applying insulation tape & placing sleeve over it. Another protective sleeve placed over the repair.\n\ninsulation tested by megger - in good condition.","2020-12-20","","Completed","2020-12-18","No","No","No","Internal"]
[null,null,null,null,17964,"26_20 Feb 2021 1:26:05 AM","2020-12-19","Observation","Ship Staff","Ship Staff Insp.","Provision Crane - observed 440 VAC low insulation alarm trigger when slewing motor is operated.","Deck - Machinery,Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","On troubleshooting found slewing motor giving low insulation; further found tell tale signs of water ingress in the motor terminal & possibly windings.\n\nAttempts to heat up motor in place did not improve the situation.\n\nMotor brought to er workshop , dismantled, cleaned & heating lamps put on - insulation improved to 55 Mohm.\n\nSlewing motor overhauled, both bearings renewed, stator cleaned with electro-solvent, dried up and boxed back. Applied silicone sealant on motor terminal to prevent water ingress.\n\nMegger test carried out - satisfactory.","2020-12-30","","Completed","2020-12-22","No","No","No","Internal"]
[null,null,null,null,17965,"26_20 Feb 2021 6:41:07 AM","2020-12-20","Observation","Ship Staff","Ship Staff Insp.","FWG ejector pump overboard valve found unable to operate. The pinion found not moving with the operating spindle.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Gear box removed & dismantled - found the pinion is broken at the locking pin. Pinion from old valve used to make it operational. Operating gear assemblyfitted back - working satisfactorily.","2020-12-31","","Completed","2020-12-22","No","No","No","Internal"]
[null,null,null,null,17973,"26_20 Feb 2021 1:33:58 AM","2020-12-20","Observation","Ship Staff","Ship Staff Insp.","Galley 440 VAC breaker at MSB tripped when hot plate switched ON","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","Found faulty thermal switch, same renewed - satisfactory.","2020-12-20","","Completed","2020-12-20","No","No","No","Internal"]
[null,null,null,null,17966,"26_20 Feb 2021 6:45:25 AM","2020-12-21","Observation","Ship Staff","Ship Staff Insp.","Main air compressor # 2 - cylinder head gasket observed damaged during operation.","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related","","","","","Damaged cylinder head gasket renewed; coolers cleaned & inspected; drain float cleaned & inspected; crankcase inspected & oil renewed. All in good order. Compressor tried out after assembly - satisfactory.","2020-12-23","","Completed","2020-12-21","No","No","No","Internal"]
[null,null,null,null,17967,"26_20 Feb 2021 6:53:55 AM","2020-12-22","Observation","Ship Staff","Ship Staff Insp.","Emergency Bilge Suction Valve connected to main SW pump did not open when 3M routine operation verification test carried out.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Emergency bilge suction valve dismantled.\n\nDeposit of mud over the valve disc prevented the disc from lifting up.\n\nValve overhauled, internal cleaned & painted; Valve fitted back & tested for operation - working satisfactory.\n\n","2020-12-24","","Completed","2020-12-22","No","No","No","Internal"]
[null,null,null,null,17968,"26_20 Feb 2021 6:57:42 AM","2020-12-26","Observation","Ship Staff","Ship Staff Insp.","Veg room temperature controller observed fluctuation in the display temperature at the controller and frequent on/off of the solenoid valve. No spare on board.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","Requisition raised.\n\nController replaced by new supply spare & initialization carried out - working satisfactory.","2021-03-25","AQUA200220","Completed","2021-01-26","No","No","No","Internal"]
[null,null,null,null,17969,"26_20 Feb 2021 7:04:48 AM","2020-12-27","Observation","Ship Staff","Ship Staff Insp.","Calorifier hot water temperature controller for electric heater observed display blinking 0 for PV & SV and no control action for heater in auto mode.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","Integrituy od connections checked - OK.\n\nVoltage to the controller checked - normal 220 VAC.\n\nController suspected defective - end of life.\n\nRequisition raised.\n\nArrangement made using timer for eye wash system for providing hot water in accommodation - working normal with timer based cut-in & cut-out of the electric heater.\n\nUpon receipt of new controller, same installed, initialization carried out & various parameters confirmed for optimum operation - working satisfactory.","2021-03-26","AQUA200219","Completed","2021-01-23","No","No","No","Internal"]
[null,null,null,null,17970,"26_20 Feb 2021 7:13:10 AM","2020-12-28","Observation","Ship Staff","Ship Staff Insp.","Accommodation AC compressor # 1 - observed V-belt broken during use - end of life. No new spare V-belts on board.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","Already raised order for 2 sets of V-belts in engine stores requisition.\n\nOld & used V-belts in workable condition fitted for running the AC compressor - working satisfactorily.","2021-03-27","AQUA200193","Completed","2020-12-28","No","No","No","Internal"]
[null,null,null,null,17913,"26_20 Feb 2021 7:20:15 AM","2020-12-28","Observation","Ship Staff","Ship Staff Insp.","Calorifier - upon failure of electric heater controller, steam heater tried out but found not working.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","To investigate for root cause among components in the circuit - temperature control valve, steam trap, steam inlet valve, condensate return valve, pipeline for any blank, etc and make system operational.","2021-06-27","","Completed","2021-02-28","No","No","No","Internal","Advice latest update and action taken so far to move this case forward."]
[null,null,null,null,17971,"26_20 Feb 2021 7:27:48 AM","2020-12-29","Observation","Ship Staff","Ship Staff Insp.","MGPS high sea suction anode current high - unable to adjust using the potentiometers for the purpose.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","Potentiometers removed from system circuit and checked to find open circuit for the mid terminal; the total resistance as measured between end terminals is about 0.76 k?.\n\nRequisition raised.\n\nNewly received potentiometers fitted by soldering for both anode circuits - working satisfactory.","2021-03-28","AQUA210001","Completed","2021-01-28","No","No","No","Internal"]
[null,null,null,null,17914,"26_20 Feb 2021 7:34:16 AM","2020-12-29","Observation","Ship Staff","Ship Staff Insp.","Calorifier steam heater - steam inlet valve and condensate return valve observed not holding. No suitable spare valve on board.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Calorifier steam heater - both steam inlet and condensate return valve renewed and working satisfactory ","2021-06-28","","Completed","2021-05-02","No","No","No","Internal","Renewal of valves is one solution, but also servicing of these valves could be another solution. WE would like to venture second option wherever feasible and possible. Rather all leaking steam valves could be serviced one by one at given opportunity."]
[null,null,null,null,17972,"26_20 Feb 2021 7:37:52 AM","2020-12-30","Observation","Ship Staff","Ship Staff Insp.","FWG ejector pump suction strainer - observed crack on body.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Casing removed & brought to ER workshop & repaired by welding using CI electrodes - working satisfactory.","2021-01-05","","Completed","2021-01-02","No","No","No","Internal"]
[null,null,null,null,17974,"26_22 Feb 2021 7:53:48 PM","2020-12-30","Observation","Ship Staff","Ship Staff Insp.","IGG instrument air pressure regulator & line filter units observed malfunction and body with cracks.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Requisition already raised.\n\nTemporary arrangement made for continued instrument air supply.\n\nDefective units replaced by new received supply, required modifications to the connections done - working satisfactory.","2021-03-29","AQUA200168","Completed","2021-02-13","No","No","No","Internal"]
[null,null,null,null,23357,"26_2 Jan 2022 8:45:37 PM","2021-01-01","Breakdown","Ship Staff","Ship Staff Insp.","During IGG in operation O2 is not constant due to sea water leakage.Inspection carried out and obserbed lealage from top welded portion and at bottom part.","Inert Gas","Cargo / Ballast Systems","Equipment Related","","","","","Repaired carried out by work shop team.Inside thickness measured and found in normal condition.Top side cleaned and TIG welding carried out. In other place SS doubler fitted and welded.Bottom part new liner fabricated and welded in place. Pump tried out no leak were obserbed. IGG tried out and found all parameters are in normal condition.","2021-12-23","","Completed","2021-12-23","No","No","No","Internal"]
[null,null,null,null,17975,"26_20 Feb 2021 7:42:38 AM","2021-01-02","Observation","Ship Staff","Ship Staff Insp.","MECC oil bunker line from port side is blocked, suspect blank in pipeline.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","MECC oil bunker taken from stbd side bunker manifold.\n\nTo check & make operational.\n\nBlank identified & removed from the pipeline - satisfactory.","2021-04-01","","Completed","2021-02-04","No","No","No","Internal"]
[null,null,null,null,17976,"26_20 Feb 2021 7:48:53 AM","2021-01-03","Observation","Ship Staff","Ship Staff Insp.","Water fountain (water cooler) in engine room - found filter deteriorated.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","No new spare on board. Requisition already raised.\n\nOld & used spare filter cartridge in workable condition fitted - working satisfactory.","2021-06-02","AQUA200206","Completed","2021-01-03","No","No","No","Internal"]
[null,null,null,null,17977,"26_21 Feb 2021 7:14:54 PM","2021-01-05","Observation","Ship Staff","Ship Staff Insp.","Fire detection system - sensor at boiler observed with deteriorated base.","LSA / FFA","Eng. / Strg. Comp.","Equipment Related","","","","","Replaced by spare base on board - working satisfactory.","2021-01-07","","Completed","2021-01-05","No","No","No","Internal"]
[null,null,null,null,17978,"26_21 Feb 2021 7:22:15 PM","2021-01-05","Observation","Ship Staff","Ship Staff Insp.","Fire Detection system - Loop O/C fault noted on display panel.","LSA / FFA","Eng. / Strg. Comp.","Equipment Related","","","","","Checked the system, \"Loop Test\" carried out - \n\non first check system gave scan result showing only left side check working for all points and no right side check made.\n\non second check, loop test scan report results fives all working fine but alarm exists.\n\nShore technician attanded vessel and after their checks rectified the fault by placing jumpers in the SCI unit at the steering flat entrance - no alarm now.\n\nSystem working normal.","2021-04-04","AQUA215020","Completed","2021-01-28","No","No","No","Internal"]
[null,null,null,null,16322,"26_18 Dec 2020 2:16:19 PM","2021-01-08","Defect","Ship Staff","Ship Staff Insp.","Steam return line for COT 3 WGS leaking and steam trap choked.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","","","","","New steam return line fabricated and steam trap replaced for COT 3WGS.","2021-03-31","","Completed","2021-04-01","No","No","No","Internal","Steam line to fabricate and renew soonest!"]
[null,null,null,null,17979,"26_21 Feb 2021 7:49:58 PM","2021-01-11","Observation","Ship Staff","Ship Staff Insp.","3/O cabin toilet light not operational - no spares on board.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","on investigation found choke faulty - no spare on board.\n\nArrangement modified to fix CFL holder & use CFL lamp on board.\n\nnew modified arrangement tested for operation - working satisfactory.","2021-01-15","","Completed","2021-01-12","No","No","No","Internal"]
[null,null,null,null,17980,"26_21 Feb 2021 8:03:08 PM","2021-01-13","Observation","Ship Staff","Ship Staff Insp.","AE # 3 - observed unit # 1 exhaust temperature very low","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","on investigation found securing bolts broken (5 out of 8) for housing roller guide.\n\nCylinder head removed to enable extraction of broken bolts by drilling.\n\nBroken bolts removed, for one observed threads are damaged, same re-tapped to next size and appropriate bolt used.\n\nAll parts cleaned and inspected - found in good working order.\n\nAll working components re-assembled and engine tried out - working satisfactory.","2021-03-12","","Completed","2021-01-17","No","No","No","Internal"]
[null,null,null,null,17981,"26_21 Feb 2021 9:06:08 PM","2021-01-14","Observation","Ship Staff","Ship Staff Insp.","Light Fixtures - at aft of accommodation noted FL lamp in burnt condition.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","Repaired same lighting fixture & converted for LED tubelight, globe renewed.\n\nnew arrangement LED light tested for operation - working satisfactory.","2021-01-21","","Completed","2021-01-14","No","No","No","Internal"]
[null,null,null,null,17982,"26_21 Feb 2021 9:12:12 PM","2021-01-15","Observation","Ship Staff","Ship Staff Insp.","Galley hot plate reported not working again","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","Found cable burnt at the terminal connection to the hot plate.\n\nBurnt wires renewed - satisfactory.","2021-01-20","","Completed","2021-01-15","No","No","No","Internal"]
[null,null,null,null,17983,"26_21 Feb 2021 8:35:34 PM","2021-01-17","Observation","Ship Staff","Ship Staff Insp.","AE # 3 turbocharger exhaust gas outlet temperature alarm trigger.","E/R - Aux. Engine,Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","On troubleshooting, observed the cable from sensor to panel has deteriorated & damaged; verified by using new cable.\n\nNew cable laid out, secured & connections made - working satisfactory.","2021-01-24","","Completed","2021-01-17","No","No","No","Internal"]
[null,null,null,null,17992,"26_21 Feb 2021 9:16:43 PM","2021-01-18","Observation","Ship Staff","Ship Staff Insp.","Aux Engine # 1 - for unit # 1 observed securing bolts slack for housing rolle guide.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Housing removed, all parts cleaned & inspected - in good working condition. Bolts were slack & none broken.\n\nAll parts re-assembled and engine tried out - satisfactory.","2021-01-31","","Completed","2021-01-20","No","No","No","Internal"]
[null,null,null,null,17984,"26_21 Feb 2021 9:33:27 PM","2021-01-22","Observation","Ship Staff","Ship Staff Insp.","Slop Tank (S) cargo discharge pump - observed discharge stopped.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","on investigation, found bundle of rags clogging at the mouth and are well inside the pump - unable to lower the pump.\n\nThe protruding rags in the suction manually cut in pieces & removed to enable lowering of the pump for dismantling.\n\nupon dismantling found pump full of rags, same removed, all parts cleaned & inspected - OK.\n\nPump assembled with new seal rings & tried out - working satisfactory.","2021-01-27","","Completed","2021-01-23","No","No","No","Internal"]
[null,null,null,null,17985,"26_21 Feb 2021 9:38:13 PM","2021-01-27","Observation","Ship Staff","Ship Staff Insp.","main engine unit # 1 - exhaust valve observed not closing.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Exhaust valve replaced by overhauled one.","2021-01-28","","Completed","2021-01-28","No","No","No","Internal"]
[null,null,null,null,17986,"26_26 Feb 2021 12:29:27 AM","2021-01-30","Observation","Ship Staff","Ship Staff Insp.","Control air system - pressure noted to be less even after renewal & optimum setting of the 30K7 pressure reducing valve.\n\nObserved the line filters in use with previous model of control air dryer are still in use.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","After discussion with office, the older line filter elements removed. System observed - working satisfactory.\n\nPresently the old housing for these filters is still in place and after monitoring it is to be replaced by fixed piping at suitable convenient opportunity.","2021-03-29","","Completed","2021-02-13","No","No","No","Internal"]
[null,null,null,null,17987,"26_21 Feb 2021 10:09:51 PM","2021-02-01","Observation","Ship Staff","Ship Staff Insp.","COT 2S pressure & temperature not displayed on monitor.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","Found dome filled with water and the terminal totally damaged together with pressure sensor.\n\nChecked all other domes - found water in domes for COT 1S, COT 4P, Slop (P) - water cleared from all domes.\n\nPressure sensor renewed for COT 2S tank - working normal.\n\non further troubleshooting for temperature display, found water ingress in junction box, same cleared & damaged cables repaired/renewed. Silicone sealant applied on sealing face of cover for junction box - working satisfactory.\n\nAll junction boxes inspected - satisfactory.\n\nThe water ingress has been after the extensive deck washing post cargo oil tank cleaning (black oil to white oil conversion).","2021-02-07","","Completed","2021-02-04","No","No","No","Internal"]
[null,null,null,null,17988,"26_22 Feb 2021 7:43:35 PM","2021-02-01","Observation","Ship Staff","Ship Staff Insp.","Anchor light reported not working.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","On investigation found water ingress in junction box, same cleared. Junction box cleaned & terminal connectors renewed. Junction boxed secured using sealant at sealing surfaces - satisfactory.\n\nLight fixture inspected, lamp renewed & boxed back using sealant - satisfactory.","2021-02-04","","Completed","2021-02-01","No","No","No","Internal"]
[null,null,null,null,17989,"26_22 Feb 2021 7:58:14 PM","2021-02-04","Observation","Ship Staff","Ship Staff Insp.","Cascade tank outlet valve observed not holding when shut for renewing valves on boiler feed water pumps.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Valve replaced by spare on board - satisfactory.","2021-02-11","","Completed","2021-02-04","No","No","No","Internal"]
[null,null,null,null,17990,"26_22 Feb 2021 8:38:08 PM","2021-02-04","Observation","Ship Staff","Ship Staff Insp.","Boiler feed water pump # 2 - suction valve found not holding.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","New valve on board - to replace the defective valve.\n\nReplaced by new supply spare.","2021-02-05","AQUA200191","Completed","2021-02-04","No","No","No","Internal"]
[null,null,null,null,17991,"26_22 Feb 2021 8:47:19 PM","2021-02-04","Observation","Ship Staff","Ship Staff Insp.","Boiler fuel oil flexible hose to burner observed with tell tale signs of leak","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","Replaced by spare flexible hose after modification to its connection as spare hose noted with different connections - satisfactory with no leaks. Anti-splash tape placed over the connection fittings.","2021-02-10","","Completed","2021-02-04","No","No","No","Internal"]
[null,null,null,null,17993,"26_22 Feb 2021 8:52:13 PM","2021-02-04","Observation","Ship Staff","Ship Staff Insp.","Boiler - observed pressure not holding when boiler is isolated. Suspect malfunction / defective bypass valve (for warm-up of steam system) to steam stop valve.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","Renewed bypass valve to steam stop valve.","2021-02-05","","Completed","2021-02-04","No","No","No","Internal"]
[null,null,null,null,17994,"26_24 Feb 2021 13:38:07","2021-02-04","Observation","Ship Staff","Ship Staff Insp.","Boiler feed water pump # 1 start push button in ECR found damaged / broken.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","Usage stopped until repaired. To replace / renew.\n\nDefective start push button renewed using spare on board.","2021-05-03","","Completed","2021-02-05","No","No","No","Internal"]
[null,null,null,null,17995,"26_24 Feb 2021 13:46:17","2021-02-04","Observation","Ship Staff","Ship Staff Insp.","During operation of provision crane observed slight lowering of 440 VAC insulation.","Deck - Machinery,Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","On investigation found power cable damaged for slewing motor.\n\nDamaged cable renewed & crane tried out - satisfactory.","2021-05-03","","Completed","2021-02-05","No","No","No","Internal"]
[null,null,null,null,17996,"26_24 Feb 2021 16:43:55","2021-02-05","Observation","Ship Staff","Ship Staff Insp.","ECR - observed insulation mat behind the main switchboard is deteriorated.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","Deteriorated mat replaced by spare certified mat on board.","2021-03-04","","Completed","2021-02-05","No","No","No","Internal"]
[null,null,null,null,17997,"26_24 Feb 2021 16:48:43","2021-02-05","Observation","Ship Staff","Ship Staff Insp.","Main engine unit # 5 - observed 2nd piston ring broken.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","To overhaul unit at first opportunity.\n\nUnit overhaul carried out. Piston replaced by spare overhauled one using new cermet type piston rings and overhauled stuffing box.\n\nMain engine tried out in ahead and astern directions from ECR & wheel house - satisfactory.","2021-02-08","","Completed","2021-02-06","No","No","No","Internal"]
[null,null,null,null,17998,"26_24 Feb 2021 16:54:17","2021-02-06","Observation","Ship Staff","Ship Staff Insp.","Stbd lifeboat engine did not start during routine checks - starter observed not engaging with the engine flywheel.","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","Starter removed - shaft & pinion cleaned & lubricated. Starter operation checked in electrical workshop using old spare battery from lifeboat - working satisfactory.\n\nStarter fitted back and operation tested - working satisfactory & engine started normal.\n\n\n\nPinion shaft for port lifeboat cleaned and lubricated as preventive measure - satisfactory.","2021-02-10","","Completed","2021-02-06","No","No","No","Internal"]
[null,null,null,null,17999,"26_24 Feb 2021 17:00:14","2021-02-06","Observation","Ship Staff","Ship Staff Insp.","Low insulation trigger on ESB due to emergency light for stbd life boat preparation faulty.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","To isolate and rectify the fault.\n\nRepaired emergency light by renewing defective cables with deteriorated insulation.","2021-02-10","","Completed","2021-02-06","No","No","No","Internal"]
[null,null,null,null,18000,"26_24 Feb 2021 17:36:44","2021-02-08","Observation","Ship Staff","Ship Staff Insp.","Ballast tank cover (1 in number) handle corroded and wasted","Hull & Tanks","Cargo / Ballast Systems","Equipment Related","","","","","New handles fabricated and fitted with fabricated securing arrangement welded on to the cover.","2021-02-09","","Completed","2021-02-08","No","No","No","Internal"]
[null,null,null,null,18001,"26_24 Feb 2021 17:41:22","2021-02-08","Observation","Ship Staff","Ship Staff Insp.","Cargo oil tank dome covers (2 in number) observed with corroded & wasted hinges","Hull & Tanks","Cargo / Ballast Systems","Equipment Related","","","","","Corroded hinges cropped and new fabricated ones welded, corroded and wasted sections repaired.","2021-02-09","","Completed","2021-02-08","No","No","No","Internal"]
[null,null,null,null,18002,"26_24 Feb 2021 17:45:01","2021-02-08","Observation","Ship Staff","Ship Staff Insp.","ESB 220 VAC low insulation trigger from stbd lifeboat launching light","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","On opening the light fixtures found the internal cables are with deteriorated insulation. Cables & holder renewed. Light fitted back - working satisfactory.","2021-02-10","","Completed","2021-02-08","No","No","No","Internal"]
[null,null,null,null,18012,"26_24 Feb 2021 17:55:49","2021-02-08","Observation","Ship Staff","Ship Staff Insp.","Lube oil purifier # 2 motor failed to run when started - gets tripped with failure alarm. Motor is already overhauled and freenees confirmed during re-installation.","E/R - Purifier,Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","To troubleshoot & rectify the fault.\n\non investigation found Timer 19T malfunctioning; no spare on board. Requisition raised.\n\nSwapped timer from # 1 unit starter - working satisfactory.\n\nLater, among old & used timers found one workable, same used for lube oil purifier # 1 - working satisfactory.","2021-05-07","AQUA210024","Completed","2021-02-08","No","No","No","Internal"]
[null,null,null,null,18003,"26_24 Feb 2021 18:01:26","2021-02-09","Observation","Ship Staff","Ship Staff Insp.","7K4 steam pressure reducing valve - observed leaking at gasket.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","To isolate and rectify.\n\nLeaky gasket renewed - satisfactory.","2021-02-15","","Completed","2021-02-09","No","No","No","Internal"]
[null,null,null,null,18004,"26_24 Feb 2021 18:15:22","2021-02-09","Observation","Ship Staff","Ship Staff Insp.","Boiler gauge glass (port) observed leaking.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","Gauge Glass isolated - to overhaul.\n\nGauge glass overhauled, body sealing surface have lots of pittings, deteriorated gaskets renewed.\n\noverhauled gauge glass fitted and place and checked - working satisfactory. After putting in use, the securing bolts tightened again as per procedure.","2021-02-15","","Completed","2021-02-09","No","No","No","Internal"]
[null,null,null,null,18005,"26_24 Feb 2021 18:19:02","2021-02-09","Observation","Ship Staff","Ship Staff Insp.","Ballast tank vent head found corroded.","Hull & Tanks","Cargo / Ballast Systems","Equipment Related","","","","","to renew wasted covers.\n\nCorroded & wasted covers renewed - satisfactory.","2021-02-10","","Completed","2021-02-09","No","No","No","Internal"]
[null,null,null,null,18006,"26_24 Feb 2021 18:26:13","2021-02-11","Observation","Ship Staff","Ship Staff Insp.","FW hydrophore pump observed it did not start after auto cut-out.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","To investigate & rectify.\n\nOn investigation found the pressure switch contact does not fully operate with drop in pressure - possible wear at the contact point.\n\nAdjustment made to the activating point (screw with locking arrangement is provided) & tested for operation - working satisfactory.","2021-05-10","","Completed","2021-02-11","No","No","No","Internal"]
[null,null,null,null,18007,"26_26 Feb 2021 12:03:28 AM","2021-02-12","Observation","Ship Staff","Ship Staff Insp.","Fuel oil auto backwash filter stopping back flushing as not able to change over candles completely.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","Back flush carried out manually.\n\non investigation found the 5/2 solenoid valve for the filter change over deteriorated.\n\n5/2 solenoid vlave overhauled using spare repair kit on board & fitted - working good.\n\nSystem restored to normal operation - satisfactory.\n\nRequisition raised for repair kits","2021-02-14","AQUA210025","Completed","2021-02-12","No","No","No","Internal"]
[null,null,null,null,17917,"26_26 Feb 2021 2:34:52 AM","2021-02-12","Observation","Ship Staff","Ship Staff Insp.","Lube oil purifier # 2 heater observed deteriorated performance.","E/R - Purifier","Eng. / Strg. Comp.","Equipment Related","","","","","Heater to open, inspect & clean.\n\nheater dismantled & removed to engine room workshop for cleaning - was found chocked with solid sludge.\n\nHeater cleaned manually & chemically.","2021-03-11","","Completed","2021-02-27","No","No","No","Internal","We consider this happened due to long haul between heater cleaning.  Suggest to follow regular cleaning routine for better performance."]
[null,null,null,null,18008,"26_26 Feb 2021 12:14:29 AM","2021-02-13","Observation","Ship Staff","Ship Staff Insp.","IGG burner nozzle found with damaged fixing screw for tightening swirl against nozzle plate.","Inert Gas","Eng. / Strg. Comp.","Equipment Related","","","","","Complete nozzle replaced by spare one on board.\n\nRequisition raised.","2021-02-20","AQUA210023","Completed","2021-02-13","No","No","No","Internal"]
[null,null,null,null,18009,"26_26 Feb 2021 12:18:36 AM","2021-02-13","Observation","Ship Staff","Ship Staff Insp.","Control air dryer - observed dryer inlet & outlet filters are interchagned as checked with the manual.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","Inlet & outlet filters removed, connection fittings reset to suit the original position as per manual.\n\nFilter element cleaned & inspected - good condition, same used & assembly fitted as per manual.\n\nRequisition raised for spare elements.","2021-02-13","AQUA210015","Completed","2021-02-13","No","No","No","Internal"]
[null,null,null,null,18010,"26_26 Feb 2021 12:46:31 AM","2021-02-13","Observation","Ship Staff","Ship Staff Insp.","Wilden pump - observed suction side has developed crack","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","Repaired using plastic putty.\n\nRequisition raised for new one.","2021-02-28","AQUA210027","Completed","2021-02-13","No","No","No","Internal"]
[null,null,null,null,18011,"26_26 Feb 2021 1:24:45 AM","2021-02-14","Observation","Ship Staff","Ship Staff Insp.","Cargo tanks high & overfill system - observed false alarm trigger when tank level are known to be well below the alarm level.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","Connections checked & tighteneed, a loosened connection was causing the alarm - working satisfactory.","2021-02-21","","Completed","2021-02-17","No","No","No","Internal"]
[null,null,null,null,18013,"26_26 Feb 2021 12:56:12 AM","2021-02-15","Observation","Ship Staff","Ship Staff Insp.","Observed FO overflow tank level increasing at rate more than normal.\n\nFuel oil auto backwash filter - drain line observed more hot and also one filter vent line was more hot than normal.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","Bypass filter put in use.\n\nDrain valve overhauled, all seal rings renewed & fitted back.\n\nFilter candles cleaned, floats removed from the casing for inspection - found one was deteriorated / damaged enough to leak when oil filled into the chamber.\n\nFloat for venting – rectified the deteriorated valve. A disc of suitable size cut from high temp rubber & glued over the deteriorated valve on float. Working satisfactory.\n\nRequisition raised","2021-05-14","AQUA210025","Completed","2021-02-15","No","No","No","Internal"]
[null,null,null,null,18014,"26_26 Feb 2021 1:15:48 AM","2021-02-17","Observation","Ship Staff","Ship Staff Insp.","Bilge Pump Tray - drain line observed to be clogged.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","To dismantle & clear the drain line.\n\nCheck valve & drain pipe removed & cleared - satisfactory.","2021-02-24","","Completed","2021-02-17","No","No","No","Internal"]
[null,null,null,null,18015,"26_26 Feb 2021 1:48:55 AM","2021-02-20","Observation","Ship Staff","Ship Staff Insp.","LT Cooler # 1 - Observed deteriorated performance.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","To dismantle and clean as lot of mud observed in the sea water at Chittagong anchorage.\n\nLT cooler opened up & manually cleaned all the plates - was filled with mud & debris. Cooler boxed up using old gaskets as no new spare found on board. Cooler put in use - working satisfactory.","2021-02-24","","Completed","2021-02-24","No","No","No","Internal"]
[null,null,null,null,18016,"26_26 Feb 2021 1:57:53 AM","2021-02-20","Observation","Ship Staff","Ship Staff Insp.","LT cooler # 2 - observed deteriorated performance.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","To dismantle and clean as lot of mud observed in the sea water at Chittagong anchorage.\n\nLT cooler opened up & manually cleaned all the plates - was filled with mud & debris. Cooler boxed up using old gaskets as no new spare found on board. Cooler put in use - working satisfactory.","2021-02-24","","Completed","2021-02-22","No","No","No","Internal"]
[null,null,null,null,17918,"26_26 Feb 2021 2:46:18 AM","2021-02-24","Observation","Ship Staff","Ship Staff Insp.","Engine Room overhead crane - Pendant control station  securing arrangement deteriorated / wasted & unable to secured.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","the two halves held together with cable tie and electrical tape used.\n\n\n\nNo spare on board. Requisition raised.\n\nReplaced by new supply spare & tried out - Satisfactory","2021-08-23","AQUA210026","Completed","2021-03-08","No","No","No","Internal","Noted. Please do needful after receiving needed item!"]
[null,null,null,null,16320,"26_24 Nov 2020 21:43:26","2021-03-30","Observation","Ship Staff","Ship Staff Insp.","EGB wash drain line to dedicated drain tank found chocked.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","All of the blocked sections cleared.\n\n\n\n","2021-06-30","","Completed","2021-05-04","No","No","No","Internal","Noted job completed and all lines are clear now."]
[null,null,null,null,19054,"26_Sun May 02 2021 11:12:02 GMT+0000","2021-04-10","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","IGG Jacket leak repairs with High Temperature Putty.","Inert Gas","Cargo / Ballast Systems","External Factors","","","","","IGG Jacket water leak repairs carried out with high temperature putty. There is no water leakages and space will be inspected on monthly basis.","2021-04-30","","Completed","2021-04-24","No","No","No","Internal","IGG Jacket water leak rectification noted; monitor space regularly and ensure putty is applied again as required. Permanent repairs is only possible during docking and job to be added to DD job specs."]
[null,null,null,null,19055,"26_Sun May 02 2021 11:19:25 GMT+0000","2021-04-10","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Steam Line derusting and coating with STEAMKOTE to complete.","Deck - Pipe / Fittings","General Appearance","External Factors","","","","","All steam pipelines now derusted and coated with STEAMKOTE.","2021-04-30","","Completed","2021-04-30","No","No","No","Internal","Job completion noted. Maintain these lines leak free and rust free."]
[null,null,null,null,19056,"26_Sun May 02 2021 11:26:35 GMT+0000","2021-04-10","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","For smooth functioning, IGG atmospheric valve pneumatic actuator valve to remove and clean.","Inert Gas","Cargo / Ballast Systems","Equipment Related","","","","","IGG atmospheric valve pneumatic actuator valve removed and cleaned.","2021-04-30","","Completed","2021-04-24","No","No","No","Internal","Noted. Now valve will function smoothly."]
[null,null,null,null,19057,"26_Sun May 02 2021 11:30:37 GMT+0000","2021-04-10","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Soot collecting tank holed drain pipe to repair.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","External Factors","","","","","Soot collecting tank cleaned and repairs carried out on corroded drain pipe.","2021-04-30","","Completed","2021-04-24","No","No","No","Internal","Noted."]
[null,null,null,null,19058,"26_Sun May 02 2021 11:30:38 GMT+0000","2021-04-10","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Soot collecting tank holed drain pipe to repair.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","External Factors","","","","","Soot collecting tank cleaned and repairs carried out on corroded drain pipe.","2021-04-30","","Completed","2021-04-24","No","No","No","Internal","Noted."]
[null,null,null,null,19059,"26_Sun May 02 2021 11:33:20 GMT+0000","2021-04-10","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","?\tAft LT cooler corroded sea water outlet pipe section to fabricate and renew at the earliest.","E/R - Pipes/ valves & fittings","Structural Condn. / WT integrity ","External Factors","","","","","?\tAft LT cooler corroded sea water outlet pipe section renewed.","2021-05-15","","Completed","2021-04-24","No","No","No","Internal","Noted."]
[null,null,null,null,19060,"26_Sun May 02 2021 11:39:29 GMT+0000","2021-04-10","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","KEW MACHINE USED FOR EGB WASHING, DECK WASHING TO MAKE OPERATIONAL.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related,External Factors","","","","","Repaired KEW machine cable connection and made operational.","2021-05-15","","Completed","2021-04-24","No","No","No","Internal","NOTED."]
[null,null,null,null,16318,"26_24 Nov 2020 20:57:20","2021-04-10","Observation","Owner / Marine / Tech. Suptd.","Ship Staff Insp.","Pressure reducing valve - hand made gasket gives way after few operations.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","After consultations with the maker, requisition raised for the part with the gasket (gasket not sold separately).\n\n\n\nMeanwhile, we continue replacing the damaged gasket with the fabricated one from sheet.","2021-06-30","AQUA215030","Completed","2021-06-30","No","No","No","Internal","REQUIRED CONSUMABLES SUPPLIED AND MAINTENANCE CARRIED OUT FOR RENEWAL OF VALVE."]
[null,null,null,null,19032,"26_30 Apr 2021 1:12:29 PM","2021-04-14","Defect","Ship Staff","Ship Staff Insp.","Echo Sounder Printer not printing properly","Navigation - Echo Sounder / Speed Log","Navigation","Equipment Related","","","","","Printer head renewed with the spare one","2021-07-14","AQUA210061","Completed","2021-05-23","No","No","No","Internal","After defect reported, Printer order was confirmed and it was tried to connect printer at previous port in Japan, however time was insufficient for supply. Now it will be arranged at next convenient port. \nTill that period, record the readings wherever necessary."]
[null,null,null,null,19040,"26_30 Apr 2021 8:48:51 AM","2021-04-14","Defect","Ship Staff","Ship Staff Insp.","Aft Spring Winch - Aft drum - Leaking from the Brake Piston and Brake Solenoid \t\t","Deck - Mooring Machinery","Mooring","Equipment Related","9.14","Medium","","","O ring for the Brake Piston was renewed and Brake Solenoid was replaced with the Spare ones","2021-07-14","","Completed","2021-04-16","No","No","No","Internal"]
[null,null,null,null,19033,"26_30 Apr 2021 8:26:31 AM","2021-04-20","Defect","Ship Staff","Ship Staff Insp.","Ballast Eductor Pipe coming from Fire line has a Hole due to which Driving pressure for eductor cannot be created\t","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.11","Medium","","","Pipe Fabricated and put back in its original position","2021-07-20","","Completed","2021-05-02","No","No","No","Internal","Job is completed as reported."]
[null,null,null,null,19034,"26_30 Apr 2021 8:22:35 AM","2021-04-25","Observation","Ship Staff","Ship Staff Insp.","Calibration bottle not available for Calibrating Portable Gas Instruments\t\t\t","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","5.23","Very High","","","Calibration Bottles supplied at Ulsan, S Korea","2021-07-25","AQUA210063","Completed","2021-05-22","No","No","No","Internal","Raise requisition and we will supply calibration gases immediately."]
[null,null,null,null,19035,"26_30 Apr 2021 8:19:26 AM","2021-04-29","Defect","Ship Staff","Ship Staff Insp.","1 Nos UTI is not in working condition. Showing \" No Msg\" on the UTI screen","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.12","Medium","","","Shore Calibration carried out \n\n","2021-07-29","AQUA210069","Completed","2021-05-24","No","No","No","Internal","Raise requisition for UTI Tape renewal and servicing, we will arrange at next convenient port."]
[null,null,null,null,19037,"26_30 Apr 2021 8:37:56 AM","2021-04-29","Defect","Ship Staff","Ship Staff Insp.","No: 5 - Stbd Side Manifold + No: 2 S COT (Drop or Discharge) + No: 5 S COT (Drop or Discharge)  Leaking\t\t","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.11","Medium","","","No: 5 Stbd (Drop + Discharge) & No:5 Manifold valve seat ring renewed. No:2 Stbd valve Re-tested during tank cleaning and found not leaking","2021-07-29","AQUA210061","Completed","2021-06-25","No","No","No","Internal","As per reporting, necessary seat rings have been renewed. Raise requisition for spare seat rings."]
[null,null,null,null,19038,"26_30 Apr 2021 8:16:50 PM","2021-04-30","Defect","Ship Staff","Ship Staff Insp.","Fixed Gas Detection System H2S sensor only showing 0.0 ppm reading. Sensor cannot be calibrated","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","5.22","High","","","H2S Sensor replaced and function test carried out","2021-07-30","","Completed","2021-06-28","No","No","No","Internal","Investigate and raise requisition for sensor if required!"]
[null,null,null,null,19778,"26_14 May 2021 8:39:49 AM","2021-05-12","Defect","Ship Staff","Ship Staff Insp.","Leak in the VRCS system of Cargo line","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.11","Medium","","","Remove the Hole section of the pipe and new pipe  inserted with the Ermeto Coupling","2021-08-12","","Completed","2021-05-14","No","No","No","Internal"]
[null,null,null,null,19779,"26_17 May 2021 07:33:33","2021-05-13","Observation","Ship Staff","Ship Staff Insp.","During routines inspection of incinerator furnace found some of re-fractory crack and fallen down  in the primary chamber   ","Elect. Mach. & Equip.","General Appearance","Equipment Related","","","","","Refractory repaired  by ship staff.","2021-08-20","","Completed","2021-07-05","No","No","No","Internal"]
[null,null,null,null,23358,"26_4 Jan 2022 11:14:52","2021-06-04","Breakdown","Ship Staff","Ship Staff Insp.","Inspected inside and found sea water leakage.Repair carried out by applying high temprature putty.","Inert Gas","Cargo / Ballast Systems","Equipment Related","","","",""," Thickness measured and found in stisfactory condition.Inspected and found crack developed  at top welded portion.TIG  welding  carried out and tried out and found in good condition.Inside the wall found five pin hole same repaired by SS doubler plate. Under part new liner fabricated and welded. IGG tried out no leak were obserbed. IGG working in good order.","2021-06-25","","Completed","2021-12-23","No","No","No","Internal"]
[null,null,null,null,17210,"26_Fri Jan 15 2021 08:07:47 GMT+0000","2021-06-30","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","WATER BALLAST TANKS ARE HEAVILY CORRODED AND NEED TO START TANK COATING UPGRADE PROJECT.","Hull & Tanks","Cargo / Ballast Systems","External Factors","","","","","WATER BALLAST TANKS INSPECTED. WORK SCOPE PREPARED.","2022-02-28","","Completed",null,"Yes","No","No","Internal","NECESSARY WORK FOR TRADING OF VESSEL IS CARRIED OUT. REST OF THE JOB TO BE CARRIED OUT IN DRYDOCK. PLEASE PREPARE DETAILED WORKSCOPE FOR EACH BALLAST TANK WITH DETAILED INSPECTION OF EACH BALLAST TANK."]
[null,null,null,null,12175,"26_5 Jun 2020 7:40:48 PM","2021-06-30","Observation","Ship Staff","Ship Staff Insp.","Mooring Winch drum brake band to be derusted.","Deck - Mooring Machinery","Mooring","Equipment Related","","","","","Aft Spring , Port and Starboard Stern line mooring winch drum brake band derusted, Brake Liners changed and Brake rendering test carried out.","2021-12-30","","Completed","2021-07-14","No","No","No","Internal","JOB COMPLETED."]
[null,null,null,null,16323,"26_30 Dec 2020 11:53:34 AM","2021-06-30","Defect","Ship Staff","Ship Staff Insp.","Emergency generator , quick closing valve box corroded with cover..","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","External Factors","","","","","Cover box  cropped and corroded portion  repaired. Box painted and installed in place.","2021-09-30","","Completed","2021-08-02","No","No","No","Internal","Even though operationally it does not interfere, have this one fixed asap."]
[null,null,null,null,20149,"26_4 Jul 2021 6:40:31 PM","2021-07-01","Defect","Ship Staff","Ship Staff Insp.","1S, 2S and 6S Temperature reading are erratic ","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.13","Medium","","","Investigate found water ingressed in temperature sensors and their terminal connectors found damaged same renewed and tried out found working good.","2021-10-01","","Completed","2021-07-06","No","No","No","Internal"]
[null,null,null,null,20147,"26_4 Jul 2021 6:36:24 PM","2021-07-02","Defect","Ship Staff","Ship Staff Insp.","2 Nos Mooring winch brake cannot be Adjusted\t","Deck - Mooring Machinery","Mooring","Equipment Related","9.14","Medium","","","Mooring winch brake handle in Frozen condition. Same removed from the location and made free","2021-10-02","","Completed","2021-08-20","No","No","No","Internal"]
[null,null,null,null,20148,"26_4 Jul 2021 6:48:12 PM","2021-07-04","Defect","Ship Staff","Ship Staff Insp.","Paint Locker Blower not in working condition\t","Deck - Machinery,LSA / FFA","Safety / LSA / FFA","Equipment Related","5.35","Medium","","","Fan motor overhauled. Fan hub was  found damaged  same has been  repaired on board. Fan  fixed and tried out. Working satisfactory.","2021-10-04","","Completed","2021-07-07","No","No","No","Internal"]
[null,null,null,null,20891,"26_1 Aug 2021 10:46:59 PM","2021-07-05","Defect","Ship Staff","Ship Staff Insp.","5S cargo tank pressure sensor reading was showing C.FAIL in CCR.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","Checked found pressure sensor good. Connections checked in the temp sensor terminal box found pressure sensor wire damaged same rectified and tried out found correct tank pressure reading is coming in CCR.","2021-08-05","","Completed","2021-07-24","No","No","No","Internal"]
[null,null,null,null,20887,"26_1 Aug 2021 10:52:23 PM","2021-07-12","Defect","Ship Staff","Ship Staff Insp.","Fixed gas detection system is showing flow fault alarm when analyzing the every sampling point.","Deck - Machinery","Cargo / Ballast Systems","Equipment Related","","","","","Checked found VS1 vacuum switch defective. Spares received in L.A. Both fitted in place and tried out working as per order.","2021-08-18","AQUA210122","Completed","2021-10-23","No","No","No","Internal","SPARES ORDERED AND WILL BE CONNECTED."]
[null,null,null,null,20897,"26_1 Aug 2021 13:22:53","2021-07-13","Defect","Ship Staff","Ship Staff Insp.","VRCS power failure alarm was comimg frequently.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","Checked found K701 relay NO auxilliary contact malfunctioning. Spare NO auxilliary contact used and tried out now system working as per order.","2021-08-05","","Completed","2021-07-22","No","No","No","Internal"]
[null,null,null,null,20892,"26_25 Jul 2021 12:37:42","2021-07-14","Defect","Ship Staff","Ship Staff Insp.","No#6 S cargo tank FRAMO p/p unable to strip the cargo.","Deck - Machinery","Cargo / Ballast Systems","Equipment Related","","","","","FRAMO cargo p/p wear ring, cargo seal and seal element renewed and tried out found satisfactory.","2021-07-25","","Completed","2021-07-22","No","No","No","Internal"]
[null,null,null,null,20893,"26_1 Aug 2021 13:06:38","2021-07-20","Breakdown","Ship Staff","Ship Staff Insp.","Hydro blaster found not working.","Deck - Machinery","General Appearance","Equipment Related","","","","","Checked found water cut out switch defective. Same received and renewed. Tried out found working in good order.","2021-08-25","AQUA210113","Completed","2021-08-16","No","No","No","Internal"]
[null,null,null,null,20894,"26_25 Jul 2021 12:31:42","2021-07-21","Breakdown","Ship Staff","Ship Staff Insp.","Incinerator primary burner motor failure","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Incinerator primary burner motor renewed with new spare onboard.","2021-08-06","AQUA210112","Completed","2021-07-21","No","No","No","Internal"]
[null,null,null,null,20895,"26_1 Aug 2021 10:41:49 PM","2021-07-21","Breakdown","Ship Staff","Ship Staff Insp.","Incinerator secondary burner motor found running on low RPM.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Checked found capacitor defective same renewed and tried out now secondary burner motor working good.","2021-07-23","","Completed","2021-07-22","No","No","No","Internal"]
[null,null,null,null,20896,"26_17 Aug 2021 14:31:04","2021-07-23","Defect","Ship Staff","Ship Staff Insp.","Sanitary exhaust blower bearings making abnormal noise.","Accommodation","General Appearance","Equipment Related","","","","","Blower dismantled. Bearings renewed. Blower boxed back and tried oiut found now working as per order.","2021-08-08","","Completed","2021-08-03","No","No","No","Internal"]
[null,null,null,null,20898,"26_16 Aug 2021 09:57:02","2021-08-06","Defect","Ship Staff","Ship Staff Insp.","Aux. boiler, FD fan linkages found broken.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","Linkages repaired.","2021-08-22","","Completed","2021-08-14","No","No","No","Internal"]
[null,null,null,null,22634,"26_5 Sep 2021 11:17:43","2021-08-13","Defect","Ship Staff","Ship Staff Insp.","COT no#2 (P) and (S) high level alarm didn’t occurred, after loading the cargo more than 95%.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","After discharging both sensors removed and found high level float has lost its buoyancy. Port side replaced with old good float and stbd side replaced with new spare. Now COT no#2 P and S high level alarm is working as per order. ","2021-09-10","","Completed","2021-09-04","No","No","No","Internal"]
[null,null,null,null,20899,"26_17 Aug 2021 14:37:05","2021-08-13","Breakdown","Ship Staff","Ship Staff Insp.","IGG O2 analyser showing zero reading while calibration.","Cargo Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Found O2 measuring cell defective same renewed with new one and calibration carried out. All working as per order.","2021-08-13","","Completed","2021-08-13","No","No","No","Internal"]
[null,null,null,null,22635,"26_5 Sep 2021 10:49:33","2021-08-15","Defect","Ship Staff","Ship Staff Insp.","ECR common and PAL not working.","Elect. Mach. & Equip.","General Appearance","Equipment Related","","","","","Checked found LAN cable in CCR switch to hub (1mtr cable) defective same renewed. Now working fine. ","2021-08-16","","Completed","2021-08-15","No","No","No","Internal"]
[null,null,null,null,20886,"26_25 Aug 2021 11:02:24","2021-08-15","Defect","Ship Staff","Ship Staff Insp.","Aft mast anchor and stern navigation light fittings broken due to vibration.","Navigation - Others","Navigation","Equipment Related,External Factors","","","","","Both light fixtures are in bad condition. spares received. Both light fittingsd renewed and tried out found working satisfactory.","2021-09-25","AQUA210129","Completed","2021-09-22","No","No","No","Internal","LIGHT FITTINGS ORDERED AND CONNECTED AT KOREA. PLEASE CARRY OUT REQUIRED MAINTENANCE AND REPLACE EXISTING UNITS WITH NEW."]
[null,null,null,null,20888,"26_17 Aug 2021 16:41:50","2021-08-16","Breakdown","Ship Staff","Ship Staff Insp.","Deck air service air compressor belt and fan broken. ","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related","","","","","Belts and Fan renewed after spares received in Hawaii.","2021-09-16","AQUA215054 &  AQUA210126","Completed","2021-08-30","No","No","No","Internal","BELT AND FANS ORDERED AND CONNECTED AT KOREA. CARRY OUT REQUIRED MAINTENANCE AND REPLACE THE PARTS."]
[null,null,null,null,20890,"26_25 Aug 2021 11:27:30","2021-08-21","Defect","Ship Staff","Ship Staff Insp.","VRCS No#2 motor was not cutting IN in auto.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","VRCS No # 2 motor repaired. Auto cut In & cut off operational.","2021-10-15","AQUA210127","Completed","2021-09-01","No","No","No","Internal","AQUA210127 SPARES ORDERED. UPON RECEIPT OF SPARES, CARRY OUT REQUIRED MAINTENANCE."]
[null,null,null,null,22636,"26_4 Oct 2021 11:23:06","2021-08-23","Breakdown,Critical Equipment","Ship Staff","Ship Staff Insp.","L/b engine(p)exhaust pipe found corroded badly.","Critical Equip.,LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","New pipe fabricated and fitted. tried out found working in good condition. No leakage found.","2021-08-23","","Completed","2021-08-23","No","No","No","Internal"]
[null,null,null,null,22620,"26_28 Sep 2021 10:52:57 AM","2021-08-24","Critical Equipment","Ship Staff","Nav Audit / Verification","MF/HF Showing Tune NG while transmiting above 4 KHZ frequency.","Navigation - GMDSS & Communication","Navigation","Equipment Related","","","","","Trouble shooting carried out as per Manfacturer & company advice. Vessel awaiting Technician/Spares. Technician attended this job and afterwards it starts working good.","2021-12-30","","Completed","2021-12-10","Yes","No","No","Internal","job completed at Singapore call around 3rd Dec"]
[null,null,null,null,20889,"26_25 Aug 2021 11:33:55","2021-08-24","Defect","Ship Staff","Ship Staff Insp.","Galley cooking range hot plate no#1 and 3 found not working in high mode.","Accommodation,Elect. Mach. & Equip.","Crew Management","Equipment Related","","","","","Hot plate no#1 checked found heat switch defective and one coil burnt. Hote plate no33 checked found one coil burnt. Both need to replace. Spares received and replaced with defective parts and tried out now cooking range working in good order.","2021-12-08","AQUA210133","Completed","2021-11-19","No","No","No","Internal","Spares supplied"]
[null,null,null,null,22646,"26_5 Sep 2021 11:10:33","2021-08-26","Breakdown","Ship Staff","Ship Staff Insp.","STP air blower motor was showing zero insulation. ","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Motor removed from place, dismantled, found water inside. Motor stator first cleaned with fresh water and then over hauled. Motor boxed back and insulation taken found 1800 mega ohm. Blower fitted in place and tried out found working well. ","2021-08-28","","Completed","2021-08-27","No","No","No","Internal"]
[null,null,null,null,22637,"26_13 Nov 2021 09:56:03","2021-08-31","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Weather tight door for Hospita retention bar wasted.","Accommodation","Structural Condn. / WT integrity ","External Factors","","","","","Wasted material(Retention bar) to renewed and then painted door portion.","2021-09-15","","Completed","2021-09-10","No","No","No","Internal"]
[null,null,null,null,22638,"26_4 Oct 2021 10:41:22","2021-09-07","Critical Equipment,Defect","Ship Staff","Ship Staff Insp.","Fire alarm manual call point “B136” was giving false fire alarm.","Critical Equip.,Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","Checked found its testing clip broken and it’s beyond repair. Hence replaced with new manual call point and tried out found working as per order","2021-09-08","","Completed","2021-09-07","No","No","No","Internal"]
[null,null,null,null,22639,"26_4 Oct 2021 10:47:42","2021-09-12","Defect","Ship Staff","Ship Staff Insp.","Cascade tank oil in water sensor tried out found not responding in oily condition.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","Sensor checked found defective same renewed with new spare sensor and tried out now sensor working as per order","2021-10-20","","Completed","2021-09-13","No","No","No","Internal"]
[null,null,null,null,22640,"26_4 Oct 2021 10:53:21","2021-09-20","Breakdown","Ship Staff","Ship Staff Insp.","Aft stern Suez light fitting found damaged and water ingresses in it.","Elect. Mach. & Equip.,Navigation - Others","Navigation","Equipment Related","","","","","Same removed, repaired and fitted back now light fitting working well","2021-09-25","","Completed","2021-09-23","No","No","No","Internal"]
[null,null,null,null,22641,"26_4 Oct 2021 11:00:36","2021-09-20","Defect","Ship Staff","Ship Staff Insp.","ECR A/C was not cutting off in H.P.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","Checked found malfunctioning of dual pressure switch same rectified and tested found L.P and H.P cut off as per order.","2021-10-17","","Completed","2021-09-28","No","No","No","Internal"]
[null,null,null,null,22623,"26_4 Oct 2021 11:08:23","2021-09-25","Breakdown","Ship Staff","Ship Staff Insp.","Middle window wiper was not working.","Elect. Mach. & Equip.,Navigation - Others","General Appearance","Equipment Related","","","","","Wiper found  jammed same removed from place. Found pulley bearing and belt worn out same  renewed. Railing checked for free movement. working good. Wiper motor cable continuity checked found cable is good. fitted back in its place.Motor checked found its defective. Motor need to replace. Motor received onboard. fitted in place and tried out found working as per order.","2021-12-30","","Completed","2021-12-20","No","No","No","Internal","Ordered and awaiting readiness . Target around mid dec on board."]
[null,null,null,null,22642,"26_25 Oct 2021 06:49:41","2021-09-26","Defect","Ship Staff","Ship Staff Insp.","Visco-therm was not working in auto.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Pilot relay overhauled and its orifice cleaned in control station. Tried out found working good in auto.","2021-11-20","","Completed","2021-10-21","No","No","No","Internal"]
[null,null,null,null,22643,"26_25 Oct 2021 07:01:08","2021-10-06","Breakdown","Ship Staff","Ship Staff Insp.","From ECR A/C compressor glass, gas leakage started.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Gas collected. Sump oil renewed. Glass thread repaired. new gas charged and tried out found no leakage in the system and working well.","2021-10-25","","Completed","2021-10-08","No","No","No","Internal"]
[null,null,null,null,23359,"26_1 Dec 2021 12:05:07 PM","2021-10-07","Critical Equipment","Ship Staff","Nav Audit / Verification","SAT-C PRINTER INOPERTAIONAL ","Navigation - GMDSS & Communication","Communication","Equipment Related","","","","","R.O raised for the same. Printer received onborad and replaced and tried out found working good.","2021-12-31","","Completed","2021-12-18","No","No","No","Internal"]
[null,null,null,null,22644,"26_25 Oct 2021 07:09:10","2021-10-07","Breakdown","Ship Staff","Ship Staff Insp.","Power pack engine no#4 was unable to start. ","Cargo Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","The DC motor starter exchange with No#3 engine, still no#4 not getting started. Pick up sensor cleaned. Actuator coil and its input supply checked found okay. Starting signal working good. Fuel line checked and there is no fuel coming in return line. Stop solenoid valve was malfunctioning. Same line purged and then tried out found started as per order. requisition raised for stop solenoid valve.","2021-10-10","AQUA210146","Completed","2021-10-08","No","No","No","Internal"]
[null,null,null,null,22624,"26_25 Oct 2021 07:14:37","2021-10-08","Breakdown","Ship Staff","Ship Staff Insp.","Alpha lubricator p/p no#1 motor tripped in overload.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Checked found motor was single phasing and it was taking high current (24A). Motor insulation taken found okay. Contactor found one main contact was malfunctioning. Contactor temporarily repaired. Tried out found working as per order. Need to replace the contactor. Requisition for contactor raised in electrical stores. Contactor received and renewed. Tried out found working satisfactory.","2021-12-16","AQUA210149 (Item no#13)","Completed","2021-11-18","No","No","No","Internal","Spares arranged and connected to vessel"]
[null,null,null,null,22645,"26_13 Nov 2021 09:13:44","2021-10-09","Defect","Ship Staff","Ship Staff Insp.","A/E#3 F.O sensor faiol alarm was coming.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Same checked and found sensor defective same renewed with new spare sensor and its dampener cleaned. Now showing correct reading.","2021-11-15","","Completed","2021-11-11","No","No","No","Internal"]
[null,null,null,null,22647,"26_25 Oct 2021 07:22:26","2021-10-10","Breakdown","Ship Staff","Ship Staff Insp.","While discharging operation in Los Angeles found IGG atmospheric valve stuck in open position.","Cargo Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","It’s I/P converter signal checked found its 20mA for closing signal. Actuator of the positioner checked found stuck. Actuator is beyond repair. Valve operated manually to continue the discharging. After finishing the discharging, new spare positioner with limit switch replaced with defective valve positioner. All the control pneumatic pipe lines modified. 02nos new pipes made for open / close operation. Valve positioner with limit switch settings carried out and calibrated as per manual instructions and IGG tried out found working as per order. For old positioner, repair kit ordered.","2021-10-13","AQUA210143","Completed","2021-10-12","No","No","No","Internal"]
[null,null,null,null,22619,"26_1 Nov 2021 10:54:15","2021-10-16","Defect","Ship Staff","Ship Staff Insp.","While drill found port life boat P.A system speaker is not working.","Elect. Mach. & Equip.,Navigation - GMDSS & Communication","Crew Management","Equipment Related","","","","","Speaker checked found its coil is broken same need to replace. Requisition raised. Spares received and replaced with defective speaker and tried out found working good.","2021-12-30","AQUA210160","Completed","2021-12-01","No","No","No","Internal","Spares ordered and ready wt Singapore with National Forwarder"]
[null,null,null,null,22648,"26_25 Oct 2021 07:25:02","2021-10-17","Defect","Ship Staff","Ship Staff Insp.","220V low insulation was coming from E/R fwd flood light ballast.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","Same renewed and tried out found low insulation gone","2021-10-17","","Completed","2021-10-17","No","No","No","Internal"]
[null,null,null,null,22626,"26_25 Oct 2021 07:30:10","2021-10-19","Breakdown","Ship Staff","Ship Staff Insp.","Fish room temperature controller was showing “Err21”. Fish room temperature was dropping and its solenoid was not energised due to this error.","Elect. Mach. & Equip.","Crew Management","Equipment Related","","","","","Found fish room evaporator sensor defective. Vessel does not have same specific protective sensor PT100. Hence different PT 100 fitted in place for temporarily purpose. Its working fine. Fish room temperature came back to normal (-18deg C). Requisition raised for the PT100 sensor for evaporator. Sensor received and replaced with teporary arranged sensor and tried out found working as per order.","2021-11-18","AQUA210144","Completed","2021-12-04","No","No","No","Internal","Spares ready and is with National freight forwarder."]
[null,null,null,null,22550,"26_Wed Nov 10 2021 11:39:16 GMT+0000","2021-10-22","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","FWG feed line found leaking, to repair","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","New pipe fabricated and fixed. No further leaks observed.","2021-12-22","","Completed","2021-11-05","No","No","No","Internal"]
[null,null,null,null,22551,"26_Wed Nov 10 2021 11:42:19 GMT+0000","2021-10-22","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Aux engine #1 fuel oil feed pump found leaking","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Pump dismantled and  found pump was leaking from Lip seal.  Casing Oring and seals renewed. Further No leaks observed.","2021-12-22","","Completed","2021-11-02","No","No","No","Internal"]
[null,null,null,null,22553,"26_Wed Nov 10 2021 11:43:52 GMT+0000","2021-10-22","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","E/R Scupper pipe found corroded and holed","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","New pipe fabricated and fixed. No leaks observed.","2021-12-22","","Completed","2021-11-08","No","No","No","Internal"]
[null,null,null,null,22555,"26_Wed Nov 10 2021 11:45:35 GMT+0000","2021-10-22","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ECR A/C not cutting off on H.P. pressure switch to change","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","New pressure switch received. Pressure switch renewed , connections verified. HP pressure trip tried out. Equipment restored in good order.","2021-12-22","","Completed","2021-10-24","No","No","No","Internal"]
[null,null,null,null,22556,"26_Wed Nov 10 2021 11:46:34 GMT+0000","2021-10-22","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Port side window wiper not working","Navigation - Others","Navigation","Equipment Related","","","","","Wiper found jammed. Same eased up with grease and lubricative solution and tried out found working satisfactory.","2021-12-22","","Completed","2021-10-24","No","No","No","Internal"]
[null,null,null,null,22557,"26_Wed Nov 10 2021 11:48:53 GMT+0000","2021-10-22","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Fwd mast steering light holder in bad shape, to renew the holder","Navigation - Others","Navigation","Equipment Related","","","","","Light fitting holder renewed.","2021-12-22","","Completed","2021-11-07","No","No","No","Internal"]
[null,null,null,null,22649,"26_14 Nov 2021 09:55:54","2021-10-22","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Fwd mast steering light holder in bad shape, to renew the holder.","Navigation - Others","Navigation","Equipment Related","","","","","Light fitting holder renewed.","2021-12-22","","Completed","2021-11-07","No","No","No","Internal"]
[null,null,null,null,22650,"26_14 Nov 2021 09:41:04","2021-10-22","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","FWG feed line found leaking, to repair.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","New pipe fabricated and fixed. No leaks observed.","2021-12-22","","Completed","2021-11-06","No","No","No","Internal"]
[null,null,null,null,22651,"26_14 Nov 2021 09:43:07","2021-10-22","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Aux engine#1 fuel oil feed p/p found leaking.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Pump leaking from Lip Seal. Pump seal renewed. Other leaks in associated piplines repaired.","2021-12-22","","Completed","2021-11-02","No","No","No","Internal"]
[null,null,null,null,22652,"26_14 Nov 2021 09:45:03","2021-10-22","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","After peak tank vent cover found corroded.","Hull & Tanks","Cargo / Ballast Systems","Equipment Related","","","","","Vent head cover fabricated and fixed in place. ","2021-12-22","","Completed","2021-11-07","No","No","No","Internal"]
[null,null,null,null,22653,"26_14 Nov 2021 09:46:50","2021-10-22","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","E/R scrupper pipe found corroded and holed.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","New pipe  fabricated and and fixed. No leaks observed.","2021-12-22","","Completed","2021-11-04","No","No","No","Internal"]
[null,null,null,null,22654,"26_14 Nov 2021 10:02:54","2021-10-22","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Fuel oil feed p/p leakig. Seal to renew.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Fuel pump with motor overhauled. Restored in good ordered. No leaks observed.","2021-12-22","","Completed","2021-11-07","No","No","No","Internal"]
[null,null,null,null,22655,"26_13 Nov 2021 10:16:16","2021-10-22","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","No:2 Manifold Valve - Port Side Broken wheel of the manifold valve to repair.\n\n","Cargo Mach.,Deck - Machinery","Cargo / Ballast Systems","Equipment Related","","","","","Broken wheel replaced with new one. Valve tested, found operational.","2021-12-22","","Completed","2021-10-25","No","No","No","Internal"]
[null,null,null,null,22656,"26_13 Nov 2021 10:06:11","2021-10-22","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Mooring winch coupling allen bolt found broken\n\n","Deck - Mooring Machinery","Mooring","Equipment Related","","","","","Coupling removed , allen key bolt replaced & fixed back. ","2021-12-22","","Completed","2021-10-27","No","No","No","Internal"]
[null,null,null,null,22657,"26_13 Nov 2021 10:02:16","2021-10-22","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Steam Observation tank side glass to fix\n\n","Deck - Machinery","Cargo / Ballast Systems","Equipment Related","","","","","Steam Observation Tank side glass fixed back, checked found intact","2021-12-22","","Completed","2021-10-25","No","No","No","Internal"]
[null,null,null,null,22658,"26_13 Nov 2021 10:10:49","2021-10-22","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","\"Void Space 6P and 6S, Manhole rubber Packing to renew\"\n\n","Hull & Tanks","Structural Condn. / WT integrity ","Equipment Related","","","","","Void Space 6P and 6S, Manhole rubber Packing to renewed.","2021-12-22","","Completed","2021-11-01","No","No","No","Internal"]
[null,null,null,null,22659,"26_13 Nov 2021 10:19:08","2021-10-22","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Forecastle Bilge Valve noted in stuck position, to renew\n\n","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","","","","","Forecastle bilge valve renewed & old valve lapping carried out.","2021-12-22","","Completed","2021-11-05","No","No","No","Internal"]
[null,null,null,null,22660,"26_13 Nov 2021 10:22:08","2021-10-22","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Foam Monitor - Port Side Accomodation valve to ease up\n\n","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","Foam Monitor - Port side Accomodation valve freed.","2021-10-30","","Completed","2021-10-24","No","No","No","Internal"]
[null,null,null,null,22661,"26_14 Nov 2021 10:04:56","2021-10-22","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Main deck - Steam line valve extended handle to fabricate and fix.","Deck - Pipe / Fittings","General Appearance","Equipment Related","","","","","Main deck - Steam line valve extended handle  fabricated and fixed back","2021-12-22","","Completed","2021-10-26","No","No","No","Internal"]
[null,null,null,null,22662,"26_14 Nov 2021 09:48:36","2021-10-22","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Deck fresh water pipe found corroded and holed.","Deck - Pipe / Fittings","General Appearance","Equipment Related","","","","","Deck fresh water pipe near Steam observation tank area abricated & fixed back.","2021-12-22","","Completed","2021-11-03","No","No","No","Internal"]
[null,null,null,null,22663,"26_14 Nov 2021 09:38:59","2021-10-22","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Main deck - Fire line found corroded, section to renew.","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","Main deck - New Fire line section from 6W's Pumpstack to 5 W's pumpstack fabricated & renewed.","2021-11-07","","Completed","2021-11-05","No","No","No","Internal"]
[null,null,null,null,22664,"26_14 Nov 2021 09:34:02","2021-10-22","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","WBT (No#2 WBT Stbd side) Tank dome cover hinges found broken, to repair.","Hull & Tanks","Cargo / Ballast Systems","Equipment Related","","","","","WBT (No#2 WBT Stbd side) Tank dome cover hinges repaired.","2021-12-22","","Completed","2021-10-24","No","No","No","Internal"]
[null,null,null,null,22665,"26_14 Nov 2021 10:00:31","2021-10-22","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Fresh water pipe pin hole leak noted on deck.","Deck - Pipe / Fittings","General Appearance","Equipment Related","","","","","Fresh water pipe line fabricated & replaced on deck near manifold area.","2021-12-22","","Completed","2021-11-10","No","No","No","Internal"]
[null,null,null,null,null,"26_Wed Nov 10 2021 11:54:36 GMT+0000","2021-10-22","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Fuel oil feed pump leaking, seal to renew","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related",null,null,"Not Applicable","Not Applicable","Fuel oil pump overhauled and mechanical seal renewed.","2022-02-28",null,"Completed","2022-03-10","No",null,null,"Internal"]
[null,null,null,null,22630,"26_1 Nov 2021 10:41:06","2021-10-23","Defect","Ship Staff","Ship Staff Insp.","440V low insulation alarm is coming from galley baking oven.","Elect. Mach. & Equip.","Crew Management","Equipment Related","","","","","Baking oven No#1 and 2 top heating elements found giving low insulation alarm and no#2 temperature controller is malfunctioning. Requisition raised for the baking oven spares. Spares received. Coil and controller renewed and oven tried oiut , now no 440V low insulation alarm is coming fro oven.","2021-11-21","AQUA210147","Completed","2021-11-19","No","No","No","Internal","Spares supplied at Yesou"]
[null,null,null,null,22666,"26_1 Nov 2021 10:34:48","2021-10-23","Defect","Ship Staff","Ship Staff Insp.","FWG Salino meter was showing false salinity reading.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","The electrodes checked found pitted. New electrode sensor found and fitted in place. Tried out found showing 2.5 PPM (Satisfactory) after few hours of running.","2021-11-15","","Completed","2021-10-26","No","No","No","Internal"]
[null,null,null,null,22669,"26_13 Nov 2021 09:02:10","2021-10-24","Defect","Ship Staff","Ship Staff Insp.","Port side ballast p/p evacuation system was not an operational.","Cargo Mach.,Deck - Machinery","Cargo / Ballast Systems","Equipment Related","","","","","Its solenoid v/v found damaged same replaced with new spare. Spool v/v overhauled. Pilot air filter cleaned and new base made for connector fitment. System tried out and working as per order. ","2021-11-10","","Completed","2021-11-08","No","No","No","Internal"]
[null,null,null,null,22667,"26_13 Nov 2021 09:15:58","2021-10-25","Defect","Ship Staff","Ship Staff Insp.","A/E#1 and 2, F.O pressure was fluctuating.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Both transmitters dampener cleaned and tried out, now working as per good order. ","2021-11-15","","Completed","2021-11-11","No","No","No","Internal"]
[null,null,null,null,22759,"26_Thu Dec 02 2021 04:01:12 GMT+0000","2021-10-25","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Accommodation Front walkway to chip, buff and paint","Miscellaneous","General Appearance","Equipment Related","","","","","Accommodation Front walkway to chipping, buffing and painting carried out","2021-12-15","","Completed","2021-11-25","No","No","No","Internal"]
[null,null,null,null,22631,"26_12 Nov 2021 09:21:05","2021-10-29","Defect","Ship Staff","Ship Staff Insp.","Compass deck P.A speaker is not working.","Deck - Machinery","General Appearance","Equipment Related","","","","","Speaker checked and found it’s defective. Requisition raised for the same. Spares received and fitted in place and tried out found working as per order.","2021-11-16","AQUA210160","Completed","2021-12-15","No","No","No","Internal","Spares ordered and ready with NF"]
[null,null,null,null,22668,"26_12 Nov 2021 09:34:36","2021-11-05","Defect","Ship Staff","Ship Staff Insp.","Vessel received an over speed trip alarm / trip on safety panel (Lyngso Marine DPS 2100. Only Tacho Pic-up Sensor 2 Fail alarm is being received. When this alarm triggers, RPM at instrument panel shows 50~60RPM. ","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Sensors cleaned. Pick-up 2 Sensor is disconnected from DMZ402 card and M/E observed for 24hours found no over speed alarm and trip activated that concluded pick-up sensor 2 is defective and giving false signal. Spare pick-up received in Yeosu. Sensor renewed and tried out, now no alarm and overspeed trip is coming. Working in good order.","2021-11-17","AQUA210167","Completed","2021-11-14","No","No","No","Internal"]
[null,null,null,null,23360,"26_3 Jan 2022 17:21:55","2021-11-16","Defect","Ship Staff","Ship Staff Insp.","Low 220V insulation alarm was coming in ESB. ","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","Checked and found it was coming from ELD-1. In ELD-1, it is coming from lighting breakers one is from ECR and electrical work shop and another one is from M/E under platform lights. 220V low insulation lights (ECR and Under M/E platform), defective wiring replaced and tried out found no low insulation alarm is coming from 220V ESB.\n\n","2021-11-20","","Completed","2021-11-17","No","No","No","Internal"]
[null,null,null,null,23361,"26_3 Jan 2022 17:31:12","2021-11-20","Breakdown","Ship Staff","Ship Staff Insp.","Vacuum p/p motor no#1 tripped.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Checked found contactor partially closed same removed and cleaned. Fitted back in place and temporarily started the p/p. After receiving the new contractor, replaced and tried out now p/p working in good order.","2021-12-30","AQUA210174","Completed","2021-12-18","No","No","No","Internal"]
[null,null,null,null,23362,"26_3 Jan 2022 17:34:54","2021-11-24","Defect","Ship Staff","Ship Staff Insp.","2P COT pressure reading was malfunctioning.","Cargo Mach.,Deck - Machinery","Cargo / Ballast Systems","Equipment Related","","","","","Checked found water ingress in the dome. Water removed and dome dried. Dome cover repaired. Silicon sealant applied and tried out found pressure reading was showing normal","2021-12-04","","Completed","2021-11-25","No","No","No","Internal"]
[null,null,null,null,23363,"26_3 Jan 2022 17:37:41","2021-11-25","Breakdown","Ship Staff","Ship Staff Insp.","Provision comp no#2 was tripped, found its contactor getting overheated and it damages the overload relay.","E/R - Aux. Mach.,Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","Both replaced with new spares ad tried out now working as per order.","2021-11-26","","Completed","2021-11-25","No","No","No","Internal"]
[null,null,null,null,24051,"26_15 Jan 2022 9:11:40 PM","2021-12-05","Observation","Ship Staff","Ship Staff Insp.","L.T.Cooler #1 & #2 sea water outlet pipe badly corroded and found leaking.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","New pipe fabricated in workshop and fitted in place.","2021-12-28","","Completed","2021-12-30","No","No","No","Internal"]
[null,null,null,null,23364,"26_3 Jan 2022 17:42:21","2021-12-10","Defect","Ship Staff","Ship Staff Insp.","Stbd side mid mast aft facing, flood light fitting was not working.","Elect. Mach. & Equip.","General Appearance","Equipment Related","","","","","Found its igniter defective same renewed and tried out now working good. ","2021-12-17","","Completed","2021-12-15","No","No","No","Internal"]
[null,null,null,null,23369,"26_3 Jan 2022 17:45:42","2021-12-18","Breakdown","Ship Staff","Ship Staff Insp.","STP air blower motor was showing zero insulation.","E/R - Aux. Mach.,Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","Blower emoved from place, dismantled, found water inside. Motor stator first cleaned with fresh water and then with electro-solve. Stator heated up and varnished applied. Motor boxed back and insulation taken found 1800 mega ohm. Blower fitted in place and tried out found working satisfactory. ","2021-12-18","","Completed","2021-12-18","No","No","No","Internal"]
[null,null,null,null,23354,"26_3 Jan 2022 17:56:39","2021-12-22","Breakdown","Ship Staff","Ship Staff Insp.","While discharging in Chittagong suddenly power failure alarm occurred on the framo control panel in CCR. Port side hydraulic system was unable to control from CCR.","Cargo Mach.,Elect. Mach. & Equip.","Cargo / Ballast Systems","Equipment Related","","","","","Checked and found port side control power unit defective in Framo control panel which is located in fire control station same replaced with lower capacity power supply unit and tried out found working fine. Same need to replace after original supplied. office supplied the same capacity PSU and fitted in place with base modification and tried out found working as per order.","2022-02-28","AQUA220008","Completed","2022-01-14","No","No","No","Internal","Order for spares to replace correct capacity"]
[null,null,null,null,23365,"26_3 Jan 2022 17:51:37","2021-12-22","Breakdown","Ship Staff","Ship Staff Insp.","Provision crane luffing motor tripped in overload safety.","Elect. Mach. & Equip.","General Appearance","Equipment Related","","","","","Motor remove from place, dismantled and found brake pad worn out with disc. Same repaired and motor overhauled. Motor assembled and fitted in place and tried out found working as per order.","2022-01-02","","Completed","2021-12-28","No","No","No","Internal"]
[null,null,null,null,24052,"26_15 Jan 2022 9:03:19 PM","2021-12-23","Observation","Ship Staff","Ship Staff Insp.","L.T.Cooler #1, sea water out let pipe  found leaking due to badly corroded.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","New pipe fabricated and fitted in place.","2021-12-28","","Completed","2021-12-30","No","No","No","Internal"]
[null,null,null,null,23366,"26_2 Jan 2022 8:17:48 PM","2021-12-25","Breakdown","Ship Staff","Ship Staff Insp.","MCSW Pump #1 found leaking badly due to muddy water.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","","","","","MCSW pump #1 dismantled for inspection and found stationary part of Mechanical seal found damaged and worn out.Shaft found heavy scoring mark in bush area. Shaft bush found worn out due to muddy water.Pump overhauled with new shaft,new mechanical seal and with new bush.wear ring found in good condition.pump assembled back and put in service and found working in good order. ","2021-12-27","MCSW","Completed","2021-12-27","No","No","No","Internal"]
[null,null,null,null,23367,"26_2 Jan 2022 8:28:48 PM","2021-12-25","Breakdown","Ship Staff","Ship Staff Insp.","EGB Circulating pump #2. During pump in operation ship staff obserbed leaking.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","","","","","EGB Circulating pump #2 dismantled for inspection and found mechanical seal and bearing were damaged.Pump assembled with nwe mechanical seal, new bearings, new Throttling bush and with new oil seal. Pump tried out and found working in good condition. Pump kept in stand by mode.","2021-12-28","","Completed","2021-12-28","No","No","No","Internal"]
[null,null,null,null,23368,"26_2 Jan 2022 6:49:50 PM","2021-12-31","Breakdown","Ship Staff","Ship Staff Insp.","MCSW PUMP#2 found leaking badly due to muddy water.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","","","","","MCSW PUMP#2 DISMANTLED FOR INSPECTION AND FOUND MECHANICAL SEAL STATIONARY PART BROKEN,DURING FURTHER INSPECTION SHAFT BUSH WORN OUT. WEAR RING FOND BADLY DAMAGED. DUE TO UNAVALIBILITY MECHANICAL SEAL OLD SEAL USED. PUMP ASSEMBLED WITH NEW BUSH AND NEW WEAR RING.PUMP TRIED OUT AND FOUND WORKING IN GOOD CONDITION.","2021-12-31","","Completed","2021-12-31","No","No","No","Internal"]
[null,null,null,null,24053,"26_16 Jan 2022 17:59:15","2022-01-03","Defect","Ship Staff","Ship Staff Insp.","Shaft earthing meter was showing no reading.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Checked found toggle switch malfunctioning same replaced with new toggle switch and tried out now working well","2022-01-06","","Completed","2022-01-04","No","No","No","Internal"]
[null,null,null,null,24063,"26_16 Jan 2022 9:56:10 AM","2022-01-04","Defect","Ship Staff","Ship Staff Insp.","No 5 Fire Isolation Valve Gland packing leakage","Deck - Pipe / Fittings","Safety / LSA / FFA","Equipment Related","","","","","Need to open and change gland packing","2022-01-06","","Completed","2022-01-06","No","No","No","Internal"]
[null,null,null,null,24054,"26_16 Jan 2022 18:08:45","2022-01-05","Defect","Ship Staff","Ship Staff Insp.","EGB circulating water p/p motor no#2 was not coming in stby while no#1 was running. ","E/R - Aux. Mach.,Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","Checked found its starter control panel defective. Same replaced with spare different model with wiring modification and tried out found working good","2022-01-12","AQUA220036","Completed","2022-01-07","No","No","No","Internal"]
[null,null,null,null,24064,"26_16 Jan 2022 18:02:14","2022-01-06","Critical Equipment","Ship Staff","Ship Staff Insp.","X-Band radar was missing the targets in three mile range.","Navigation - RADAR","Navigation","Equipment Related","","","","","Radar magnetron unit removed from place, replaced with new magnetron and fitted back and tried out found working as per order.","2022-01-07","AQUA220031","Completed","2022-01-07","No","No","No","Internal"]
[null,null,null,null,24055,"26_16 Jan 2022 18:25:28","2022-01-11","Defect","Ship Staff","Ship Staff Insp.","2S ballast water tank level gauging sensor was showing full in empty condition.","Cargo Mach.,Elect. Mach. & Equip.","Cargo / Ballast Systems","Equipment Related","","","","","Amplifier checked found working good. Entered in tank sensor removed from place, cleaned and fitted back and zero adjusted in empty tank and tried out found working in good order. ","2022-01-20","","Completed","2022-01-15","No","No","No","Internal"]
[null,null,null,null,24056,"26_18 Feb 2022 9:26:42 PM","2022-01-11","Observation","Ship Staff","Ship Staff Insp.","While pump running vibration obserbed.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","","","","","Pump dismantled for inspectionand found impeller and wear ring had heavy pitting. Shaft bush found worn out to excess. Mechanical seal found damaged. Pump overhauled with new impeller,new mechanical seal,new wear ring and with new shaft bush. Pump tried out found ,efficiency improved and running in good order.","2022-01-20","","Completed","2022-01-23","No","No","No","Internal"]
[null,null,null,null,24057,"26_23 Jan 2022 18:57:11","2022-01-17","Breakdown","Ship Staff","Ship Staff Insp.","440V low insulation came and Exhaust gas boiler p/p no#1 tripped in overload safety and System automatically started the No#2 pump.","E/R - Aux. Mach.,Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","Motor insulation taken found zero M?. And coupling found damaged. Motor removed from place, Dismantled and tried to overhauled the motor so that insulation can improve. After overhauling the motor, insulation checked found still zero M?. Coupling repaired. Motor rewinding carried out by shore and motor tried out found taking 8.6A (Rated amp: 10A)which is good.","2022-02-15","","Completed","2022-02-05","No","No","No","Internal"]
[null,null,null,null,null,"26_29 Jan 2022 16:29:31","2022-01-18","Breakdown","Ship Staff","Ship Staff Insp.","When tried to changed over the domestic fridge from no#2 to no#1, found no#1 compressor was not able to build the temperature in the meat and fish room after 5 days. After again changing over to the no#2 compressor the system works fine. Need to check the no#1 compressor.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related",null,null,"Not Applicable","Not Applicable","Routine maintenance carried out for No 1 Ref compressor- Checks made on Oil level , gas level , leak test , belt tension,expansion valves, foundation tightness checked.  Compressor put into service - working satisfactory.","2022-05-30",null,"Completed","2022-03-22","No",null,null,"Internal"]
[null,null,null,null,24058,"26_23 Jan 2022 19:02:11","2022-01-19","Breakdown","Ship Staff","Ship Staff Insp.","Due to fresh water generator ejector p/p motor, vessel received the 440V low insulation alarm and motor suddenly tripped in overload safety.","E/R - Aux. Engine,Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","Motor insulation taken found more than 4000M?. Motor removed from place and brought to workshop for repairs. Motor dismantled and found NDE side bearing was not good. And due to that motor rotor was touching the stator inner York part. Motor overhauled. Both bearings renewed. Motor assembled and fitted back. Starter panel checked and found main three phase line insulation was in bad condition and main line was touching the contactor control voltage line due to overheating. Same temporarily rectified by putting extra insulation. Main contactor overhauled. Motor tried out and it was kept under observation for two days and it was working as per good order.","2022-01-21","","Completed","2022-01-19","No","No","No","Internal"]
[null,null,null,null,24059,"26_29 Jan 2022 16:32:46","2022-01-19","Defect","Ship Staff","Ship Staff Insp.","Air con no#1 condenser inlet valve found leaking.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Temporarily repaired. ","2022-02-10","","Completed","2022-01-19","No","No","No","Internal"]
[null,null,null,null,24060,"26_31 Jan 2022 13:36:25","2022-01-29","Defect","Ship Staff","Ship Staff Insp.","STP air blower was making sound.","E/R - Aux. Mach.,Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","Motor with blower emoved, dismantled. Bearings found bad same renewed, blower boxed back, fitted in place and tried out now no abnormal noise is coming from blower.","2022-01-30","","Completed","2022-01-29","No","No","No","Internal"]
[null,null,null,null,24061,"26_13 Feb 2022 19:07:49","2022-02-03","Defect","Ship Staff","Ship Staff Insp.","Galley exhaust blower was making abnormal noise.","Accommodation","General Appearance","Equipment Related","","","","","Motor overhauled. faulty bearings renewed. Blower tried out and found no abnormal noise coming from it.","2022-02-10","","Completed","2022-02-07","No","No","No","Internal"]
[null,null,null,null,24062,"26_17 Feb 2022 3:24:54 PM","2022-02-04","Observation","Ship Staff","Ship Staff Insp.","On deck air line leaking.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","","","","","Open air line flange to flange and brought to engine work shop and fabricated new pipe line.","2022-02-08","","Completed","2022-02-07","No","No","No","Internal"]
[null,null,null,null,24065,"26_17 Feb 2022 3:29:17 PM","2022-02-10","Observation","Ship Staff","Ship Staff Insp.","During normal operation observed no#1 fresh water hydrophore pump leaking from gland.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","","","","","Hydrophore pump no#1 dismantled for inspection and found mechanical seal spring broken. Stationery and rotary part of seal found worn out. Rectified by replacing new mechanical seal, pump tried out and found working in good order.","2022-02-12","","Completed","2022-02-11","No","No","No","Internal"]
[null,null,null,null,24066,"26_13 Feb 2022 19:14:56","2022-02-10","Defect","Ship Staff","Ship Staff Insp.","220V low insulation alarm was coming from M.S.B.","Accommodation,Elect. Mach. & Equip.","General Appearance","Equipment Related","","","","","Checked found coming from LD-3 panel in accommodation. It found in pantry light fitting same converted into the LED light fitting and checked found no insulation in 220V feeder panel","2022-02-11","","Completed","2022-02-10","No","No","No","Internal"]
[null,null,null,null,null,"26_9 Mar 2022 7:45:39 PM","2022-03-05","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Both S band and X band radar target is missing intermittently, inspite visually sighting of target","Navigation - RADAR","Navigation","Equipment Related",null,null,"Not Applicable","Not Applicable","Magnetron replaced and modification done as per the office guideliness.","2022-05-31",null,"Completed","2022-03-26","No",null,null,"Internal"]
[null,null,null,null,null,"26_9 Mar 2022 7:34:56 PM","2022-03-05","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Main LO Auto backwash not turning","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related",null,null,"Not Applicable","Not Applicable","ME LO AUTOBACK WASH FILTER HYDRAULIC MOTOR OVERHAULED ","2022-05-31",null,"Completed","2022-03-20","No",null,null,"Internal"]

{"sheet":"Calc","index":2,"n_rows":28,"n_cols":12,"rows_kept":28,"cut":false,"hidden":true,"merged":[]}
["Def_type","Def_cause","Equipments","VIQrefno","Observer_code"]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,"Dim itemSele As Long"]
[null,null,null,null,null,null,null,null,null,null,null,"   dim startRow as integer"]
[null,null,null,null,null,null,null,null,null,null,null,"   startRow=1"]
[null,null,null,null,null,null,null,null,null,null,null,"        For itemSele = 0 To ListBox1.ListCount - 1"]
[null,null,null,null,null,null,null,null,null,null,null,"        If ListBox1.Selected(itemSele) = True Then"]
[null,null,null,null,null,null,null,null,null,null,null,"        Worksheets(\"WorksheetName\").Range(\"A\" & startRow).Value = ListBox1.List(itemSele)"]
[null,null,null,null,null,null,null,null,null,null,null,"        startRow = startRow + 1"]
[null,null,null,null,null,null,null,null,null,null,null,"        End If"]
[null,null,null,null,null,null,null,null,null,null,null,"        Next"]
[null,null,null,null,null,null,null,null,null,null,null,"Dim LastRowA As String"]
[null,null,null,null,null,null,null,null,null,null,null,"        Dim itemSele As Long"]
[null,null,null,null,null,null,null,null,null,null,null,"       Dim startRow as integer"]
[null,null,null,null,null,null,null,null,null,null,null,"        LastRowA = ActiveSheet.Cells(Rows.count, \"A\").End(xlUp).row"]
[null,null,null,null,null,null,null,null,null,null,null,"        startQue = 0"]
[null,null,null,null,null,null,null,null,null,null,null,"        For itemSele = 0 To ListBox1.ListCount - 1"]
[null,null,null,null,null,null,null,null,null,null,null,"        For startRow = 1 To LastRowA"]
[null,null,null,null,null,null,null,null,null,null,null,"        If Worksheets(\"WorksheetName\").Range(\"A\" & startRow).Value = ListBox1.List(itemSele) Then"]
[null,null,null,null,null,null,null,null,null,null,null,"        ListBox1.Selected(itemSele) = True"]
[null,null,null,null,null,null,null,null,null,null,null,"        Exit For"]
[null,null,null,null,null,null,null,null,null,null,null,"        End If"]
[null,null,null,null,null,null,null,null,null,null,null,"        Next j"]
[null,null,null,null,null,null,null,null,null,null,null,"        Next"]
[null,null,null,null,null,null,null,null,null,null,null,"        End If"]

{"sheet":"Areaofobs","index":3,"n_rows":17,"n_cols":2,"rows_kept":17,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Cargo / Ballast Systems",11]
["Cert. & Docu.",2]
["Communication",6]
["Crew Management",3]
["Emgcy. Systems",13]
["Eng. / Strg. Comp.",14]
["General Appearance",15]
["Ice Opns.",17]
["ISM Related",7]
["ISPS Related",10]
["MARPOL Related",9]
["MLC Related",4]
["Mooring",12]
["Navigation",5]
["Safety / LSA / FFA",8]
["Structural Condn. / WT integrity ",16]

{"sheet":"Vessel_type","index":4,"n_rows":1,"n_cols":2,"rows_kept":1,"cut":false,"hidden":true,"merged":[]}
["Vessel_type","ID"]

{"sheet":"Deficiency_type","index":5,"n_rows":8,"n_cols":3,"rows_kept":8,"cut":false,"hidden":true,"merged":[]}
["TITLE","Type of deficiency_description","ID"]
["Breakdown",null,6]
["Critical Equipment",null,4]
["Defect",null,1]
["Guarantee Claim",null,8]
["Non Conformity",null,2]
["Observation",null,3]
["Other",null,7]

{"sheet":"VIQrefno","index":6,"n_rows":427,"n_cols":3,"rows_kept":427,"cut":false,"hidden":true,"merged":[]}
["VIQ_ref_no","Risk Value of observation","ID"]
["1.1","Low",8243]
["1.10","Low",8252]
["1.11","Low",8253]
["1.12","Low",8254]
["1.13","Low",8255]
["1.14","Low",8256]
["1.15","Low",8257]
["1.16","Low",8259]
["1.17","Low",8260]
["1.18","Low",8261]
["1.19","Low",8262]
["1.2","Low",8244]
["1.20","Low",8263]
["1.21","Low",8265]
["1.22","Low",8266]
["1.23","Low",8267]
["1.24","Low",8268]
["1.25","Low",8269]
["1.26","Low",8270]
["1.3","Low",8245]
["1.4","Low",8246]
["1.5","Low",8247]
["1.6","Low",8248]
["1.7","Low",8249]
["1.8","Low",8250]
["1.9","Low",8251]
["1.99","High",11258]
["10.1","Medium",8461]
["10.10","High",8470]
["10.11","Medium",8471]
["10.12","Very High",8472]
["10.13","Very High",8473]
["10.14","Medium",8474]
["10.15","Low",8475]
["10.16","Very High",8476]
["10.17","Very High",8477]
["10.18","High",8478]
["10.19","Very High",8479]
["10.2","Low",8462]
["10.20","High",8480]
["10.21","Medium",8481]
["10.22","Low",8482]
["10.23","Medium",8483]
["10.24","Low",8484]
["10.25","Very High",8485]
["10.26","High",8486]
["10.27","Medium",8487]
["10.28","Low",8488]
["10.29","Medium",8489]
["10.3","Medium",8463]
["10.30","High",8490]
["10.31","Very High",8491]
["10.32","Very High",8492]
["10.33","High",8493]
["10.34","High",8494]
["10.35","Very High",8495]
["10.36","Very High",8496]
["10.37","Medium",8497]
["10.38","Medium",8498]
["10.39","High",8499]
["10.4","High",8464]
["10.40","Medium",8500]
["10.41","Medium",8501]
["10.42","Medium",8502]
["10.43","Medium",8503]
["10.44","Medium",8504]
["10.45","Very High",8505]
["10.46","High",8506]
["10.47","Medium",8507]
["10.48","High",8508]
["10.49","Medium",8509]
["10.5","Low",8465]
["10.50","High",8510]
["10.51","Low",8511]
["10.52","Medium",8512]
["10.53","Medium",8513]
["10.54","High",8514]
["10.55","Low",8515]
["10.6","Very High",8466]
["10.7","Medium",8467]
["10.8","Medium",8468]
["10.9","Medium",8469]
["10.99","High",8516]
["11.1","High",8420]
["11.10","Medium",8429]
["11.11","Very High",8430]
["11.12","Low",8431]
["11.13","Low",8432]
["11.14","Medium",8433]
["11.15","Low",8434]
["11.16","Low",8435]
["11.17","Low",8436]
["11.2","Medium",8421]
["11.3","Medium",8422]
["11.4","Very High",8423]
["11.5","Medium",8424]
["11.6","Medium",8425]
["11.7","High",8426]
["11.8","Low",8427]
["11.9","Low",8428]
["11.99","High",8437]
["12.1","High",8438]
["12.10","High",8448]
["12.11","High",8449]
["12.12","High",8450]
["12.13","High",8451]
["12.14","High",8452]
["12.15","High",8453]
["12.16","High",8454]
["12.17","High",8455]
["12.18","High",8456]
["12.19","High",8457]
["12.2","High",8439]
["12.20","High",8458]
["12.21","High",8459]
["12.3","High",8441]
["12.4","High",8442]
["12.5","High",8443]
["12.6","High",8444]
["12.7","High",8445]
["12.8","High",8446]
["12.9","High",8447]
["12.99","High",8460]
["2.1","Very High",8296]
["2.1.9","Very High",11259]
["2.10","Medium",8304]
["2.11","Medium",8305]
["2.12","Low",8306]
["2.13","Low",8307]
["2.14","Low",8308]
["2.15","Low",8309]
["2.16","Medium",8310]
["2.2","Medium",8297]
["2.3","High",8295]
["2.4","Medium",8298]
["2.5","Medium",8299]
["2.6","Low",8300]
["2.7","High",8301]
["2.8","High",8302]
["2.9","Medium",8303]
["2.99","High",8311]
["3.1","High",8312]
["3.2","Very High",8313]
["3.3","High",8314]
["3.4","Low",8294]
["3.5","Medium",8315]
["3.6","High",8316]
["3.7","Very High",8317]
["3.8","Very High",8318]
["3.99","High",8319]
["4.1","High",8320]
["4.10","High",8329]
["4.11","Medium",8330]
["4.12","Very High",8331]
["4.13","Very High",8332]
["4.14","Very High",8333]
["4.15","Very High",8334]
["4.16","Very High",8335]
["4.17","Very High",8336]
["4.18","Very High",8337]
["4.19","Low",8338]
["4.2","Medium",8321]
["4.20","Very High",8339]
["4.21","High",8340]
["4.22","Low",8341]
["4.23","High",8342]
["4.24","High",8343]
["4.25","Low",8344]
["4.26","Low",8345]
["4.27","High",8346]
["4.3","Medium",8322]
["4.4","High",8323]
["4.5","Very High",8324]
["4.6","Medium",8325]
["4.7","High",8326]
["4.8","Medium",8327]
["4.9","Medium",8328]
["4.99","High",8347]
["5.1","Very High",8517]
["5.10","High",8526]
["5.11","Low",8527]
["5.12","Medium",8528]
["5.13","High",8529]
["5.14","Very High",8530]
["5.15","Medium",8531]
["5.16","Very High",8532]
["5.17","Very High",8533]
["5.18","High",8534]
["5.19","Medium",8535]
["5.2","Very High",8518]
["5.20","Medium",8536]
["5.21","Medium",8537]
["5.22","High",8539]
["5.23","Very High",8540]
["5.24","Very High",8541]
["5.25","Medium",8542]
["5.26","Medium",8543]
["5.27","Medium",8544]
["5.28","Very High",8545]
["5.29","High",8546]
["5.3","Low",8519]
["5.30","High",8547]
["5.31","High",8548]
["5.32","High",8549]
["5.33","High",8550]
["5.34","Low",8551]
["5.35","Medium",8552]
["5.36","Low",8553]
["5.37","Low",8554]
["5.38","High",8555]
["5.39","Very High",8556]
["5.4","High",8520]
["5.40","Very High",8557]
["5.41","Very High",8558]
["5.42","Medium",8559]
["5.43","High",8560]
["5.44","High",8561]
["5.45","Medium",8564]
["5.46","Medium",8565]
["5.47","Medium",8566]
["5.48","Medium",8567]
["5.5","Low",8521]
["5.6","Low",8522]
["5.7","Medium",8523]
["5.8","Medium",8524]
["5.9","Very High",8525]
["5.99","High",8568]
["6.1","Medium",8348]
["6.10","Low",8357]
["6.11","High",8358]
["6.12","Medium",8359]
["6.13","Low",8360]
["6.14","High",8361]
["6.15","High",8362]
["6.16","Very High",8363]
["6.17","Very High",8364]
["6.18","Medium",8365]
["6.19","Low",8366]
["6.2","High",8349]
["6.20","Medium",8367]
["6.21","High",8368]
["6.22","Medium",8369]
["6.3","Low",8350]
["6.4","High",8351]
["6.5","Medium",8352]
["6.6","Medium",8353]
["6.7","High",8354]
["6.8","High",8355]
["6.9","Low",8356]
["6.99","High",8370]
["7.1","High",8371]
["7.10","High",8380]
["7.11","High",8381]
["7.12","High",8382]
["7.13","Medium",8383]
["7.14","Medium",8384]
["7.15","High",8385]
["7.16","High",8386]
["7.17","High",8387]
["7.2","High",8372]
["7.3","Low",8373]
["7.4","Low",8374]
["7.5","Low",8375]
["7.6","Medium",8376]
["7.7","Low",8377]
["7.8","High",8378]
["7.9","High",8379]
["7.99","High",8388]
["8.1","Very High",8569]
["8.10","Very High",8578]
["8.100","Low",11227]
["8.101","Medium",11228]
["8.102","Low",11229]
["8.103","Low",11230]
["8.104","Low",11231]
["8.105","Medium",11232]
["8.106","Medium",11233]
["8.107","Low",11234]
["8.108","High",11235]
["8.109","Very High",11236]
["8.11","Medium",8579]
["8.110","High",11237]
["8.111","Medium",11238]
["8.112","High",11239]
["8.113","Medium",11240]
["8.114","Low",11241]
["8.115","High",11242]
["8.116","Medium",11243]
["8.117","Medium",11244]
["8.118","Medium",11245]
["8.119","High",11246]
["8.12","Medium",8580]
["8.120","High",11247]
["8.121","Medium",11248]
["8.122","High",11249]
["8.123","High",11250]
["8.124","Low",11251]
["8.125","High",11252]
["8.126","Medium",11253]
["8.127","Medium",11254]
["8.13","Medium",8581]
["8.14","Very High",8582]
["8.15","High",8583]
["8.16","Very High",8584]
["8.17","Low",8585]
["8.18","High",8586]
["8.19","High",8587]
["8.199","High",11255]
["8.2","Medium",8570]
["8.20","Medium",8588]
["8.21","High",8589]
["8.22","Very High",8590]
["8.23","Medium",8591]
["8.24","Medium",8592]
["8.25","Very High",8593]
["8.26","High",8594]
["8.27","Medium",8595]
["8.28","Medium",8596]
["8.29","High",8598]
["8.3","Very High",8571]
["8.30","High",8599]
["8.31","High",8600]
["8.32","Low",8601]
["8.33","Medium",8602]
["8.34","High",8603]
["8.35","Medium",8604]
["8.36","Medium",8605]
["8.37","High",8607]
["8.38","Medium",8608]
["8.39","Medium",8609]
["8.4","Medium",8572]
["8.40","High",8610]
["8.41","Medium",8611]
["8.42","Medium",8612]
["8.43","Very High",8613]
["8.44","High",8615]
["8.45","High",8616]
["8.46","Very High",8617]
["8.47","Very High",8618]
["8.48","Medium",8619]
["8.49","High",8620]
["8.5","Very High",8573]
["8.50","Medium",8621]
["8.51","Low",8622]
["8.52","Low",8623]
["8.53","Low",8624]
["8.54","High",8625]
["8.55","Low",11182]
["8.56","Medium",11183]
["8.57","Medium",11184]
["8.58","High",11185]
["8.59","High",11186]
["8.6","Medium",8574]
["8.60","High",11187]
["8.61","Medium",11188]
["8.62","Very High",11189]
["8.63","High",11190]
["8.64","Medium",11191]
["8.65","Low",11192]
["8.66","High",11193]
["8.67","High",11194]
["8.68","High",11195]
["8.69","Medium",11196]
["8.7","High",8575]
["8.70","Medium",11197]
["8.71","Very High",11198]
["8.72","Medium",11199]
["8.73","Medium",11200]
["8.74","High",11201]
["8.75","Medium",11202]
["8.76","Medium",11203]
["8.77","Medium",11204]
["8.78","Medium",11205]
["8.79","Medium",11206]
["8.8","Medium",8576]
["8.80","Medium",11207]
["8.81","Low",11208]
["8.82","Medium",11209]
["8.83","Low",11210]
["8.84","Low",11211]
["8.85","Medium",11212]
["8.86","Medium",11213]
["8.87","Medium",11214]
["8.88","Low",11215]
["8.89","High",11216]
["8.9","High",8577]
["8.90","High",11217]
["8.91","High",11218]
["8.92","Medium",11219]
["8.93","Low",11220]
["8.94","Low",11221]
["8.95","Medium",11222]
["8.96","Medium",11223]
["8.97","Low",11224]
["8.98","High",11225]
["8.99","Medium",11226]
["9.1","Low",8390]
["9.10","Medium",8399]
["9.11","Medium",8400]
["9.12","Medium",8401]
["9.13","Low",8402]
["9.14","Medium",8403]
["9.15","Medium",8404]
["9.16","High",8405]
["9.17","High",8406]
["9.18","Low",8407]
["9.19","Low",8408]
["9.2","Very High",8391]
["9.20","Medium",8409]
["9.21","Medium",8410]
["9.22","Low",8411]
["9.23","Low",8412]
["9.24","Medium",8413]
["9.25","Low",8414]
["9.26","Low",8415]
["9.27","Low",8416]
["9.28","Medium",8417]
["9.29","Low",8418]
["9.3","Very High",8392]
["9.4","High",8393]
["9.5","High",8394]
["9.6","Low",8395]
["9.7","Medium",8396]
["9.8","Medium",8397]
["9.9","Medium",8398]
["9.99","High",8419]

{"sheet":"Equipment_list","index":7,"n_rows":28,"n_cols":3,"rows_kept":28,"cut":false,"hidden":true,"merged":[]}
["TITLE","Equipment_list_description","ID"]
["Accommodation",null,12]
["Cargo Mach.",null,13]
["Critical Equip.",null,16]
["Deck - Machinery",null,18]
["Deck - Mooring Machinery",null,15]
["Deck - Pipe / Fittings",null,20]
["Documentation",null,21]
["E/R - Air Comp.",null,8]
["E/R - Aux. Engine",null,4]
["E/R - Aux. Mach.",null,7]
["E/R - Boiler",null,5]
["E/R - Main Engine",null,3]
["E/R - Pipes/ valves & fittings",null,9]
["E/R - Pumps",null,32]
["E/R - Purifier",null,6]
["Elect. Mach. & Equip.",null,10]
["Hull & Tanks",null,19]
["Inert Gas",null,14]
["LSA / FFA",null,17]
["Miscellaneous",null,22]
["Navigation - DGPS / EPFS / AIS",null,28]
["Navigation - ECDIS",null,25]
["Navigation - Echo Sounder / Speed Log",null,26]
["Navigation - GMDSS & Communication",null,23]
["Navigation - Others",null,11]
["Navigation - RADAR",null,24]
["Navigation - VDR / BNWAS",null,30]

{"sheet":"PSC_MOU","index":8,"n_rows":11,"n_cols":3,"rows_kept":11,"cut":false,"hidden":true,"merged":[]}
["TITLE","PSC_MOU_description","ID"]
["Asia and the Pacific",null,2]
["Caribbean",null,4]
["Europe and the North Atlantic",null,1]
["Latin America",null,3]
["The Black Sea region",null,6]
["The Indian Ocean",null,8]
["The Mediterranean",null,7]
["The Riyadh MoU",null,9]
["USCG",null,10]
["West and Central Africa",null,5]

{"sheet":"Inspection_type","index":9,"n_rows":13,"n_cols":2,"rows_kept":13,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Bunkering Audit",14]
["Cargo Audit",17]
["Engineering Audit",16]
["ISM Audit",2]
["ISPS Audit",3]
["IT Audit",10]
["MLC Audit",1]
["Mooring Audit",9]
["Nav Audit / Verification",8]
["Onboard Training",18]
["Ship Staff Insp.",15]
["Suptd. Insp.",13]

{"sheet":"Deficiency_Cause","index":10,"n_rows":8,"n_cols":3,"rows_kept":8,"cut":false,"hidden":true,"merged":[]}
["TITLE","Deficiency_Cause_description","ID"]
["Behaviour Based",null,1]
["Equipment Related",null,4]
["External Factors",null,5]
["Human Error",null,7]
["Inappropriate Procedure",null,8]
["Industry Issue",null,6]
["Knowledge Based",null,3]

{"sheet":"Observer_code","index":11,"n_rows":3,"n_cols":3,"rows_kept":3,"cut":false,"hidden":true,"merged":[]}
["TITLE","Observer_code_description","ID"]
["Owner / Marine / Tech. Suptd.",null,3]
["Ship Staff",null,2]

{"sheet":"Status_code","index":12,"n_rows":6,"n_cols":3,"rows_kept":6,"cut":false,"hidden":true,"merged":[]}
["TITLE","Status_code_description","ID"]
["Completed",null,6]
["Deferred to D D",null,5]
["In progress",null,3]
["Not Started",null,2]
["Waiting spare",null,4]

{"sheet":"PSC_ref_no","index":13,"n_rows":19,"n_cols":2,"rows_kept":19,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Alarms",9]
["Cargo operations including equipment",7]
["Certificates & Documentation",2]
["Dangerous Goods",13]
["Emergency Systems",5]
["Fire safety",8]
["ISM",16]
["ISPS",17]
["Life saving appliances",12]
["MLC, 2006",18]
["Other",19]
["Pollution Prevention",15]
["Propulsion and auxiliary machinery",14]
["Radio communication",6]
["Safety of Navigation",11]
["Structural condition",3]
["Water/Weathertight condition",4]
["Working and Living Conditions",10]

{"sheet":"Risk_value_of_obs","index":14,"n_rows":1,"n_cols":2,"rows_kept":1,"cut":false,"hidden":true,"merged":[]}
["Risk Value of observation","ID"]

{"sheet":"Year","index":15,"n_rows":18,"n_cols":1,"rows_kept":18,"cut":false,"hidden":true,"merged":[]}
["Year"]
[2014]
[2015]
[2016]
[2017]
[2018]
[2019]
[2020]
[2021]
[2022]
[2023]
[2024]
[2025]
[2026]
[2027]
[2028]
[2029]
[2030]

{"sheet":"Month","index":16,"n_rows":13,"n_cols":1,"rows_kept":13,"cut":false,"hidden":true,"merged":[]}
["Month"]
["Jan"]
["Feb"]
["Mar"]
["Apr"]
["May"]
["Jun"]
["Jul"]
["Aug"]
["Sep"]
["Oct"]
["Nov"]
["Dec"]

{"sheet":"Date_","index":17,"n_rows":32,"n_cols":1,"rows_kept":32,"cut":false,"hidden":true,"merged":[]}
["Date"]
["01"]
["02"]
["03"]
["04"]
["05"]
["06"]
["07"]
["08"]
["09"]
[10]
[11]
[12]
[13]
[14]
[15]
[16]
[17]
[18]
[19]
[20]
[21]
[22]
[23]
[24]
[25]
[26]
[27]
[28]
[29]
[30]
[31]

{"sheet":"Sheet1","index":18,"n_rows":24,"n_cols":6,"rows_kept":24,"cut":false,"hidden":true,"merged":[]}
[]
[null,"ID","E",null,"Date Recorded",1]
[null,"UNIQUE ID","F",null,"Type of Deficiency",2]
[1,"Date Recorded","G",null,"Observer code",3]
["ignore","Vessel Type","H",null,"Type of Inspection",4]
[null,"Internal / External","I",null,"Description of Deficiency",5]
[null,"Drydock","J",null,"Equipment Categories",6]
[null,"Information Sharing","K",null,"Area of Observation",7]
[null,"Critical_item","L",null,"Deficiency Cause",8]
[null,"Deficiency Type","M",null,"VIQ Ref Number",9]
[null,"Deficiency Cause","N",null,"Risk Value of Obs",10]
[null,"Inspection Type","O",null,"PSC Ref Number",11]
[null,"Equipments","P",null,"PSC MOU ID",12]
[null,"VIQ Reference Number","Q",null,"Action Taken or Required",13]
[null,"Risk Value of the observation","R",null,"Target Date",14]
[null,"PSC Reference Number","S",null,"PO Ref No.",15]
[null,"PSC MOU","T",null,"Status Code",16]
[null,"Observer Code","U",null,"Date Completed",17]
[null,"Target Date","V",null,"Drydock",18]
[null,"Status Code","W",null,"Info Sharing",19]
[null,"Description of Deficiency","X",null,"Critical Item Flag",20]
[null,"Action taken / required","Y",null,"Audit Type",21]
[null,"PO ref no","Z"]
[null,"Date completed","AA"]

{"sheet":"Ship_information","index":19,"n_rows":2,"n_cols":3,"rows_kept":2,"cut":false,"hidden":true,"merged":[]}
["Ship_ID","Ship_Name","FILE_NAME"]
["26","AQUARIUS (10-03-2022)","26_1646906197129.xlsm"]

{"sheet":"External_Deficiency_type","index":20,"n_rows":5,"n_cols":3,"rows_kept":5,"cut":false,"hidden":true,"merged":[]}
["TITLE","Type of deficiency_description","ID"]
["Condn of Class / Memo",null,5]
["Defect",null,1]
["Non Conformity",null,2]
["Observation",null,3]

{"sheet":"External_Inspection_type","index":21,"n_rows":11,"n_cols":2,"rows_kept":11,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Cargo Audit",17]
["Flag State Insp.",5]
["ISM Audit",2]
["ISPS Audit",3]
["MLC Audit",1]
["Nav Audit / Verification",8]
["OM Insp. (Eg. SIRE / CDI etc.)",6]
["Others (Eg. Insurance etc.)",12]
["PSC Inspection",4]
["Terminal Insp.",11]

{"sheet":"External_Observer_code","index":22,"n_rows":7,"n_cols":3,"rows_kept":7,"cut":false,"hidden":true,"merged":[]}
["TITLE","Observer_code_description","ID"]
["Class Surveyor",null,4]
["FSC Inspector",null,5]
["Others (Eg. Insurance etc.)",null,9]
["PSC Insp.",null,6]
["SIRE / CDI Insp.",null,8]
["Terminal Insp.",null,7]

{"sheet":"Sheet Version","index":23,"n_rows":2,"n_cols":2,"rows_kept":2,"cut":false,"hidden":true,"merged":[]}
["Version","Title"]
["2.0","Version 2.0"]