{"text_format":"1","workbook":"xlsx","n_sheets":24,"sheets":["Mainsheet","Completed","Calc","Areaofobs","Vessel_type","Deficiency_type","VIQrefno","Equipment_list","PSC_MOU","Inspection_type","Deficiency_Cause","Observer_code","Status_code","PSC_ref_no","Risk_value_of_obs","Year","Month","Date_","Sheet1","Ship_information","External_Deficiency_type","External_Inspection_type","External_Observer_code","Sheet Version"],"not_rendered":{"charts":0,"images":5,"macros":1,"external_links":0,"defined_names":12,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Mainsheet","index":0,"n_rows":28,"n_cols":28,"rows_kept":28,"cut":false,"hidden":false,"merged":[[10,8,10,9],[10,12,10,13],[12,6,12,27],[8,6,8,27]]}
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,"Defect - Damage Monitoring Sheet"]
[]
[null,null,null,null,null,null,null,"Date of Report","21-Mar-2022",null,null,"Ship Name","DHT REDWOOD (04-03-2022)"]
[]
[null,null,null,null,null,null,"VERSION : 2.0"]
[]
[]
[]
[null,null,null,null,"ID","UNIQUE ID","Date Recorded","Type of Deficiency","Observer code","Type of Inspection","Description of Deficiency","Equipment Categories","Area of Observation","Deficiency Cause","VIQ Ref Number","Risk Value of Obs","PSC Ref Number","PSC MOU ID","Action Taken or Required","Target Date","PO Ref No.","Status Code","Date Completed","Drydock","Info Sharing","Critical Item","Audit Type","Superintendent Remarks"]
[null,null,null,null,24394,"54_18/03/2022 5:33:31 AM","2020-03-30","Defect","Ship Staff","Ship Staff Insp.","EGCS SCRUBBER TRIPS INADVERTENTLY, WITHOUT WARNING ON COMMUNICATION FAILURE BETWEEN RANDOM CABINETS","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","IN CONVERSATION WITH MAKERS SINCE DELIVERY. CABLES RENEWED, VIVRATION MOUNTS INSTALLED, CONNECTORS TIGHTENED. STILL AWAITING SOLUTION.","2022-12-31","","In progress",null,"No","No","No","Internal"]
[null,null,null,null,24392,"54_17/03/2022 7:27:43 AM","2021-12-06","Defect","Ship Staff","Ship Staff Insp.","FW tank level guage leaking- to be renewed after procuring same.","Hull & Tanks","Eng. / Strg. Comp.","Equipment Related","","","","","ordered New gauge vide RO DRED 220010","2022-07-31","DRED220010 DATED 10TH JANUARY","Waiting spare",null,"No","No","No","Internal"]
[null,null,null,null,24397,"54_17/03/2022 9:12:36 AM","2022-01-27","Defect","Ship Staff","Ship Staff Insp.","NO. 2 LP SOOTBLOWER PROBLEM WITH SIGNAL FROM PLC","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","WHEN INITIALIZING, OTHER SB DO A SOFTWARE INITIALIZE WHILE NO.2 LP MOVES A FEW DEGREES AND STOPS. WHEN RUNNING IT OVERSHOOTS THE STOP POSITION OF THE CAM. SUSPECT SIGNAL ERROR FROM PLC WHILE INITIALIZING. HELP SOUGHT FROM MAKER","2022-06-30","","In progress",null,"No","No","No","Internal"]
[null,null,null,null,24153,"54_01/03/2022 09:12:51 AM","2022-02-26","Observation","Ship Staff","Ship Staff Insp.","Mushroom vent for Emergency generator room corroded and holed.","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","Equipment Related","11.7","High","","","Derust the vent and renew the wasted section of vent","2022-03-30","","In progress",null,"No","No","No","Internal"]
[null,null,null,null,24398,"54_18/03/2022 6:31:53 AM","2022-03-08","Observation","Ship Staff","Ship Staff Insp.","IGG O2 INDICATOR DISPLAY MODULE FAULTY","Inert Gas","Eng. / Strg. Comp.","Equipment Related","","","","","RO RAISED  FOR NEW DISPLAY VIDE DRED 220053","2022-06-30","DRED220053","In progress",null,"No","No","No","Internal"]
[null,null,null,null,null,"54_10/04/2022 4:19:12 PM","2022-04-10","Defect","Ship Staff","Ship Staff Insp.","STEERING GEAR SUPPLY FAN MOTOR STARTER MODULE DEFECTIVE .","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related",null,null,"Not Applicable","Not Applicable","INSTALLED SIMILER TYPE MODULE TO START THE FAN BUT HEATER CONNECTIONS NOT CONNECTED DUE TO DIFFRENT TYPE.SPARES ARE ON ORDER ","2022-05-30","DRED220068","Waiting spare",null,"No",null,null,"Internal"]
[null,null,null,null,null,"54_12/04/2022 2:29:39 PM","2022-04-12","Defect","Ship Staff","Ship Staff Insp.","DRAFT MIDSHIP STBD SIDE NOT SHOWING READING.","Cargo Mach.,Deck - Machinery,Elect. Mach. & Equip.","Cargo / Ballast Systems","Equipment Related",null,null,"Not Applicable","Not Applicable","TROUBLESHOOTING CARRIED OUT AND FOUND TRANSMITTER PCB AND TRANSDUCER NOT RESPONDING ,VESSEL DO NOT HAVE SPARES TO RECTIFY THE CAUSE.SPARES ORDERED.","2022-05-30","DRED220070","Waiting spare",null,"No",null,null,"Internal"]
[null,null,null,null,null,"54_15/04/2022 12:46:29 PM","2022-04-13","Defect","Ship Staff","Ship Staff Insp.","E/R local fire fighting system soft starter not working properly,stoping starting interminently.","LSA / FFA","Eng. / Strg. Comp.","Equipment Related",null,null,"Not Applicable","Not Applicable","troubleshooting carried out and found soft starter malfunctioning.vessel do not have soft starter onboard ,spares are on order.","2022-05-30","DRED220071","Waiting spare",null,"No",null,null,"Internal"]
[null,null,null,null,null,"54_15/04/2022 12:51:42 PM","2022-04-14","Defect","Ship Staff","Ship Staff Insp.","NO 2 AC Oil pressure transmiter defective,AC plant tripping on low oil press.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related",null,null,"Not Applicable","Not Applicable","troubleshooting carried out and found transmitter defective,vessel do not have spare and same requisition will be making foir spares.","2022-05-30",null,"In progress",null,"No",null,null,"Internal"]
[null,null,null,null,null,"54_15/04/2022 12:56:11 PM","2022-04-15","Defect","Ship Staff","Ship Staff Insp.","found radio telephone unit JSB-196GM on GMDSS console not switching ’ ON ‘ on DC supply as we switched  ‘OFF ‘AC supply .suspecting issues with the radiotelephone unit.","Navigation - GMDSS & Communication","Communication","Equipment Related",null,null,"Not Applicable","Not Applicable","Informed to Electrical technical dept.vessel tried to troubleshoot the issue and suspecting radiotelephone unit defective.communication with office in progress for rectifying the trouble.","2022-05-30",null,"In progress",null,"No",null,null,"Internal"]
[null,null,null,null,null,"54_15/04/2022 2:43:19 PM","2022-04-15","Defect","Ship Staff","Ship Staff Insp.","NO 1 SVR (ALARM MONITORING SYSTEM) CPU SWITCHING OFF AUTOMATICALLY.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related",null,null,"Not Applicable","Not Applicable","TROUBLESHOOTING CARRIED OUT AND FOUND THAT THE CPU IS MALFUNCTIONING ,SAME NEED TO BE REPLACED.","2022-05-30",null,"In progress",null,"No",null,null,"Internal"]

{"sheet":"Completed","index":1,"n_rows":529,"n_cols":28,"rows_kept":529,"cut":false,"hidden":false,"merged":[[10,8,10,9],[10,12,10,13],[12,6,12,27],[8,6,8,27]]}
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,"Defect - Damage Monitoring Sheet"]
[]
[null,null,null,null,null,null,null,"Date of Report","21-Mar-2022",null,null,"Ship Name","DHT REDWOOD (04-03-2022)"]
[]
[null,null,null,null,null,null,"VERSION : 2.0"]
[]
[]
[]
[null,null,null,null,"ID","UNIQUE ID","Date Recorded","Type of Deficiency","Observer code","Type of Inspection","Description of Deficiency","Equipment Categories","Area of Observation","Deficiency Cause","VIQ Ref Number","Risk Value of Obs","PSC Ref Number","PSC MOU ID","Action Taken or Required","Target Date","PO Ref No.","Status Code","Date Completed","Drydock","Info Sharing","Critical Item","Audit Type","Superintendent Remarks"]
[null,null,null,null,605,"54_Sat Oct 12 2019 14:09:57 GMT+0000","2018-01-18","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Isolated rust marks observed on pipe stacks – particualry on the stbd side Ballast tank IG pipe at the bottom/resting on supports","Deck - Pipe / Fittings","General Appearance","Equipment Related","","","","","To ensure maintenance is carried out immediately on observing isolated rust spots. Update as on 29 Mar: Cosmetic maintenance ongoing, new locations keep coming up for maintenance and same being undertaken asap. This job is being closed out as the locations observed by Suptd have already been attended to and cosmetics completed. ","2019-03-18","","Completed","2019-03-29","No","No","No","Internal"]
[null,null,null,null,606,"54_Tue Dec 10 2019 14:13:11 GMT+0000","2018-01-18","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Cargo manifold platform Gratings rusted","Deck - Pipe / Fittings","General Appearance","External Factors","","","","","Port side manifold gratings is  hyblasted and cosmetic maintenance is completed.","2019-04-29","","Completed","2019-05-30","No","No","No","Internal"]
[null,null,null,null,624,"54_Sat Oct 12 2019 16:55:17 GMT+0000","2018-04-06","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Minute holes observed in wire mess of 4P, 2P, 1P and Slop-S PV valves","Deck - Pipe / Fittings","General Appearance","External Factors","","","","","Flame screens of 1P and 4P were found to be having very miniscule holes and renewed. Also, these flamescreens have a dual screen protection for the purpose of spark arresting. And the condition of the secondary inner flame screen is good, without any holes.","2019-04-15","","Completed","2019-04-13","No","No","No","Internal"]
[null,null,null,null,621,"54_Sat Oct 12 2019 16:45:03 GMT+0000","2018-04-07","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Cleaning require around all sounding pipes in engine room bilges and deck as old oil not cleaned around them","Hull & Tanks","General Appearance","Human Error","","","","","All soundings pipes already painted","2019-04-15","","Completed","2019-04-08","No","No","No","Internal"]
[null,null,null,null,623,"54_Sat Oct 12 2019 16:50:44 GMT+0000","2018-04-07","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Printer for CCR pressure transmitter having faded printouts","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","Printouts for CCR pressure transmitter were still ligible and readable. However ribbon changed on 8-Apr-2019","2019-04-15","","Completed","2019-04-08","No","No","No","Internal"]
[null,null,null,null,2457,"54_14/10/2019 11:23:24 PM","2018-08-04","Defect","Ship Staff","Ship Staff Insp.","BWTS IGS SYSTEM INOPERATIONAL\t","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","System is being replaced in dry-dock and office has informed to close out this item from DDRL","2019-10-15","","Completed","2019-07-31","No","No","No","Internal"]
[null,null,null,null,2435,"54_14/10/2019 09:44:01 PM","2018-09-15","Other","Ship Staff","Ship Staff Insp.","HYDROBLASTER ROTATING NOZZLE INOPERATIONAL","Miscellaneous","General Appearance","Equipment Related","","","","","R.O. FOR NEW ROTATING NOZZLE RAISED. AS PER VFF, WILL BE READY FOR DELIVERY ARND 15-FEB-19","2019-04-15","","Completed","2019-04-19","No","No","No","Internal"]
[null,null,null,null,6281,"54_15/11/2019 09:12:42 AM","2018-11-14","Breakdown","Ship Staff","Ship Staff Insp.","Forward electric whistle motor breakdown.","Navigation - Others","Navigation","Equipment Related","4.7","High","","","Complete motor assembly replaced.","2020-03-15","DRED190226","Completed","2020-03-12","No","No","No","Internal","spares ready will be supplied at next opportunity."]
[null,null,null,null,2437,"54_14/10/2019 09:49:22 PM","2018-11-17","Defect","Ship Staff","Ship Staff Insp.","\"Port side midship draft guage inaccurate reading upto 2.0 mtrs inaccuracy","Critical Equip.","Cargo / Ballast Systems","Equipment Related","","","","","\"Replaced new sensor for the port side midship draft guage. reading in order .","2019-04-15","DRED190008","Completed","2019-05-27","No","No","No","Internal"]
[null,null,null,null,2470,"54_14/10/2019 11:53:11 PM","2018-12-08","Defect","Ship Staff","Ship Staff Insp.","M/E viscometer not working in auto mode.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","upon investigation noticed that Interface unit box pcb found faulty. Spares received and same replaced and made operational.","2019-07-15","DRED190002","Completed","2019-09-02","No","No","No","Internal"]
[null,null,null,null,2314,"54_17/10/2019 12:43:46 PM","2018-12-09","Defect","Ship Staff","Ship Staff Insp.","A/E viscometer not working in auto mode","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.37","Medium","","","NEW VISCOSENCE 3 INTERFACE BOX INSTALLED AND CONNECTED FOUND WORKING.","2019-11-15","DRED190060","Completed","2019-11-29","No","No","No","Internal"]
[null,null,null,null,2422,"54_14/10/2019 8:56:29 PM","2018-12-31","Defect","Ship Staff","Ship Staff Insp.","Deck light switch panel 2 in nos switch defective ","Elect. Mach. & Equip.","General Appearance","Equipment Related","","","","","complete switch box renewed and same working now.","2019-04-15","DRED 190052","Completed","2019-04-22","No","No","No","Internal"]
[null,null,null,null,7475,"54_Sat Oct 12 2019 06:22:45 GMT+0000 (Coordinated Universal Time)","2019-01-01","Defect","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","Both port and starboard lifeboats were not manoeuvred in the water at intervals of no more than 3 months. As per the records on board, both boats had been manoeuvred in the water on 1 November 2018 and previous to that was on 4 July 2018. Comments for postponing of the lifeboat waterborne on the deck log book dated 3 Oct 2018 were sighted. (VIQ 5.29)","LSA / FFA","Safety / LSA / FFA","External Factors","5.29","High","","","Appropriate entry for postponing of the lifeboat waterborne drill mentioned on the deck log book dated 3 Oct 2018.","2019-01-01","","Completed","2019-01-01","No","No","No","External"]
[null,null,null,null,2368,"54_13/10/2019 10:00:04 PM","2019-01-02","Defect","Ship Staff","Ship Staff Insp.","M/E unit no.7 exhaust valve,minor oil leakage from top part.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Unit no.7 exhaust valve top part removed,o-ring renewed.","2019-01-07","","Completed","2019-01-05","No","No","No","Internal"]
[null,null,null,null,2367,"54_13/10/2019 9:55:30 PM","2019-01-05","Critical Equipment","Ship Staff","Ship Staff Insp.","15 PPM Bilgemon Battery low (battery change alarm).","E/R - Aux. Mach.","MARPOL Related","Equipment Related","10.32","Very High","","","No spare battery on board req to raise same ","2019-01-20","","Completed","2019-01-05","No","No","No","Internal"]
[null,null,null,null,593,"54_Thu Oct 10 2019 15:48:45 GMT+0000","2019-01-05","Other","Ship Staff","Ship Staff Insp.","Forward CCTV Camera unit's PAN and TILT unit and zoom in/out function are in-operational.","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","Camera has been replaced due to zooming problem. Camera tried out, all functions are normal","2019-02-28","","Completed","2019-01-15","No","No","No","Internal"]
[null,null,null,null,2375,"54_14/10/2019 5:18:47 AM","2019-01-07","Defect","Ship Staff","Ship Staff Insp.","Main L.O. purifier heater not able to maintain temp.","E/R - Purifier","Eng. / Strg. Comp.","Equipment Related","","","","","Heater cleaned manually and boxed back","2019-01-20","","Completed","2019-01-11","No","No","No","Internal"]
[null,null,null,null,7484,"54_Tue Nov 12 2019 05:21:39 GMT+0000 (Coordinated Universal Time)","2019-01-08","Defect","PSC Insp.","PSC Inspection","Bothside Doors on Bridge cannot closed tightly.","Accommodation","General Appearance","Inappropriate Procedure","12.7","High","Water/Weathertight condition","","Packing was immediately readjusted to make the doors air/gas tight. This was shown to the PSC inspector and he closed the deficiency prior leaving the vessel. Code 10 was entered against Action Taken, indicating deficiency is closed.","2019-01-08","","Completed","2019-01-08","No","No","No","Internal"]
[null,null,null,null,2374,"54_14/10/2019 5:17:01 AM","2019-01-08","Defect","Ship Staff","Ship Staff Insp.","Bridge window wiper blades broken","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","Window wiper blades changed.","2019-01-20","","Completed","2019-01-14","No","No","No","Internal"]
[null,null,null,null,584,"54_Thu Oct 10 2019 14:07:25 GMT+0000","2019-01-08","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Bridge window wiper blades broken","Navigation - Others","Navigation","Equipment Related","","","","","Window wiper blades renewed","2019-01-14","","Completed","2019-01-14","No","No","No","Internal"]
[null,null,null,null,2387,"54_14/10/2019 5:47:23 AM","2019-01-08","Defect","Ship Staff","Ship Staff Insp.","Kyma UPS not working  ","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","UPS fitted with 2 new and one old battery","2019-01-20","DRED190005","Completed","2019-02-06","No","No","No","Internal"]
[null,null,null,null,7482,"54_Tue Nov 12 2019 05:13:26 GMT+0000 (Coordinated Universal Time)","2019-01-10","Defect","Ship Staff","Ship Staff Insp.","Magnetic Compass Deviation card to be made by Shore Adjuster 2 yearly.","Navigation - Others","Navigation","Equipment Related","4.13","Very High","","","Shore adjuster arranged at Singapore on 18th Jan 2019, for carrying out the magnetic compass magnets adjustment and draw deviation card.","2019-01-19","","Completed","2019-01-18","No","No","No","Internal"]
[null,null,null,null,2372,"54_14/10/2019 5:14:19 AM","2019-01-10","Defect","Ship Staff","Ship Staff Insp.","Aux boiler gauge glass leaking","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","Same removed and overhauled.","2019-01-20","","Completed","2019-01-12","No","No","No","Internal"]
[null,null,null,null,2373,"54_14/10/2019 5:15:46 AM","2019-01-11","Defect","Ship Staff","Ship Staff Insp.","D/G #1 air leaking from turbocharger","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","gasket found broken. Same replaced with new one","2019-01-20","","Completed","2019-01-13","No","No","No","Internal"]
[null,null,null,null,588,"54_Thu Oct 10 2019 15:30:17 GMT+0000","2019-01-14","Defect","Ship Staff","Ship Staff Insp.","VECS control box at the manifold found badly corroded and with rust stains all over the box","Deck - Pipe / Fittings","General Appearance","Equipment Related","","","","","Cosmetic upgradation carried out. New oxygen sensor replaced, Calibrated & tested, working in good condition","2019-01-30","","Completed","2019-01-28","No","No","No","Internal"]
[null,null,null,null,589,"54_Thu Oct 10 2019 15:33:21 GMT+0000","2019-01-14","Defect","Ship Staff","Ship Staff Insp.","General housekeeping on deck and in stores found to be lacking standards.","Miscellaneous","General Appearance","Industry Issue","","","","","All stores to be properly arranged and houskeeping to be improved significantly to maintain high standards  in safety and quality","2019-01-30","","Completed","2019-01-29","No","No","No","Internal"]
[null,null,null,null,591,"54_Thu Oct 10 2019 15:39:18 GMT+0000","2019-01-14","Defect","Ship Staff","Ship Staff Insp.","Deck seal safety breather valve found in bad condition, with flanges & nutbolts rusted and flame screen broken","Inert Gas","Cargo / Ballast Systems","Equipment Related","","","","","Flame screen renewed","2019-01-31","","Completed","2019-01-17","No","No","No","Internal"]
[null,null,null,null,594,"54_Thu Oct 10 2019 15:53:26 GMT+0000","2019-01-14","Defect","Ship Staff","Ship Staff Insp.","/ All mooring winches relief valves found painted and frozen.","Deck - Mooring Machinery","Mooring","Equipment Related","","","","","All relief valves to be made free of paint and ensure that they are working in good order","2019-01-31","","Completed","2019-01-30","No","No","No","Internal"]
[null,null,null,null,597,"54_Thu Oct 10 2019 18:27:00 GMT+0000","2019-01-14","Defect","Ship Staff","Ship Staff Insp.","Wheels of deck air and fresh water suply valves found badly wasted and corroded","Deck - Pipe / Fittings","General Appearance","Equipment Related","","","","","Same to be replace with new wheels.","2019-02-15","","Completed","2019-01-30","No","No","No","Internal"]
[null,null,null,null,601,"54_Thu Oct 10 2019 18:47:53 GMT+0000","2019-01-14","Defect","Ship Staff","Ship Staff Insp.","Protective plate for cables on the P/S L/B davit found to be corroded and wasted.","Deck - Pipe / Fittings","General Appearance","External Factors,Inappropriate Procedure","","","","","Plate to be renewed and fixed ","2019-03-15","","Completed","2019-02-28","No","No","No","Internal"]
[null,null,null,null,604,"54_Tue Dec 10 2019 14:06:18 GMT+0000","2019-01-14","Breakdown","Ship Staff","Ship Staff Insp.","No.2P bunker tank vent saveall found corroded at the lip, same to be repaired. Also all Savealls on deck to be inspected for lips plate wastage and refman made.","Deck - Pipe / Fittings","MARPOL Related","Equipment Related","","","","","No other saveall lips found corroded, all in satisfactory condition.","2019-03-30","","Completed","2019-03-29","No","No","No","Internal"]
[null,null,null,null,7445,"54_Tue Dec 10 2019 14:17:07 GMT+0000","2019-01-18","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Gun retaining springs missing on Foam monitors #3, #4, #5 ","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","Foam monitor missing springs renewed.","2019-03-30","DRED190054","Completed","2019-05-30","No","No","No","Internal"]
[null,null,null,null,2343,"54_2019-12-10 14:09:57.000","2019-01-18","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Isolated rust marks observed on pipe stacks – particualry on the stbd side Ballast tank IG pipe at the bottom/resting on supports","Deck - Pipe / Fittings","General Appearance","Equipment Related","","","","","To ensure maintenance is carried out immediately on observing isolated rust spots. Update as on 29 Mar: Cosmetic maintenance ongoing, new locations keep coming up for maintenance and same being undertaken asap. This job is being closed out as the locations observed by Suptd have already been attended to and cosmetics completed. ","2019-03-18","","Completed","2019-03-29","No","No","No","Internal"]
[null,null,null,null,2344,"54_2019-10-12 14:13:11.000","2019-01-18","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Cargo manifold platform Gratings rusted","Deck - Pipe / Fittings","General Appearance","External Factors","","","","","Port side manifold gratings is  hyblasted and cosmetic maintenance is completed.","2019-04-29","","Completed","2019-05-30","No","No","No","Internal"]
[null,null,null,null,2369,"54_14-10-2019 05:16:03","2019-01-18","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Spare Liner on Funnel platform.To be stowed in a safe place inside ER or any safe location","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Spare liner on funnel plateform already secured and there is no place IN ENGINE ROOM TO KEEP SAME. At present ther are three liners in engine room as spare.","2019-02-17","","Completed","2019-01-18","No","No","No","Internal"]
[null,null,null,null,2370,"54_14-10-2019 05:18:26","2019-01-18","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Spares to order for upcoming D/G #2 decarb","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","To raise R.O.and same raised","2019-02-02","DRED190047","Completed","2019-01-24","No","No","No","Internal"]
[null,null,null,null,2371,"54_14-10-2019 05:21:31","2019-01-18","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","No spare cartridge for T/C onboard","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","To raise R.O.and same raised","2019-02-17","DRED190048","Completed","2019-01-24","No","No","No","Internal"]
[null,null,null,null,2376,"54_14/10/2019 5:21:54 AM","2019-01-18","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","None of the gauge glass blow down/drain cock (on LP drum), remote release wire mechanism working ","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","All cocks eased up and greased","2019-02-07","","Completed","2019-01-24","No","No","No","Internal"]
[null,null,null,null,585,"54_Thu Oct 10 2019 14:11:01 GMT+0000","2019-01-18","Other","Ship Staff","Ship Staff Insp.","Bridge wing both sides water pot for wet temp was found empty","Miscellaneous","Navigation","Human Error","","","","","Water pot for the muslin cloth was immediately filled up. Prudent watch keeping to be followed always.","2019-01-18","","Completed","2019-01-18","No","No","No","Internal"]
[null,null,null,null,2377,"54_14/10/2019 5:23:54 AM","2019-01-18","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ER PIPE / FITGS\tA/C #2 CW pressure gauge not working","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Pressure gauge changed","2019-01-25","","Completed","2019-01-19","No","No","No","Internal"]
[null,null,null,null,586,"54_Thu Oct 10 2019 14:34:40 GMT+0000","2019-01-18","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Brake band opening stopper bolts, Clearance more than 10 mm","Deck - Mooring Machinery","Mooring","Equipment Related","","","","","Clearance to be maintained not more 5 mm. Same carried out","2019-01-25","","Completed","2019-01-24","No","No","No","Internal"]
[null,null,null,null,2378,"54_14/10/2019 5:27:08 AM","2019-01-18","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","A/C #2 CW pressure gauge not working","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Pressure gauge changed","2019-01-25","","Completed","2019-01-19","No","No","No","Internal"]
[null,null,null,null,587,"54_Thu Oct 10 2019 15:27:19 GMT+0000","2019-01-18","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Weekly deck water washing regimen/routines not followed ","Deck - Pipe / Fittings","General Appearance","Human Error","","","","","Same to be followed on a weekly basis","2019-01-25","","Completed","2019-01-26","No","No","No","Internal"]
[null,null,null,null,2379,"54_14/10/2019 5:28:25 AM","2019-01-18","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Refer compressor #2 CW gauge showing wrong reading","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Checked pressure transmitter and  gauge renewed.","2019-01-25","","Completed","2019-01-20","No","No","No","Internal"]
[null,null,null,null,2380,"54_14/10/2019 5:29:43 AM","2019-01-18","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Small leak from HFO Purifier#2 sampling line","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Leak rectified.","2019-01-25","","Completed","2019-01-20","No","No","No","Internal"]
[null,null,null,null,2381,"54_14/10/2019 5:30:59 AM","2019-01-18","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Both main boilers gauge glass blow down remote release wire siezed","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","Wire eased up and greased.","2019-01-27","","Completed","2019-01-24","No","No","No","Internal"]
[null,null,null,null,590,"54_Thu Oct 10 2019 15:36:14 GMT+0000","2019-01-18","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Pump room air damper remote stops cabin not water proof, water observed collected inside","Cargo Mach.","Cargo / Ballast Systems","External Factors","","","","","To check coaming sealing/packing and renew/repair as necessary","2019-02-02","","Completed","2019-01-26","No","No","No","Internal"]
[null,null,null,null,2382,"54_14/10/2019 5:32:14 AM","2019-01-18","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Hyd bracing bolts/supports on stabd side observed oil leakage","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Leakage rectified.","2019-01-27","","Completed","2019-01-25","No","No","No","Internal"]
[null,null,null,null,2383,"54_14/10/2019 5:36:32 AM","2019-01-18","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","No spare plunger/barrel for fuel pump","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","To raise R.O.and same raised","2019-02-02","DRED190046","Completed","2019-01-19","No","No","No","Internal"]
[null,null,null,null,592,"54_Thu Oct 10 2019 15:43:25 GMT+0000","2019-01-18","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Stbd gangway wire reel drum bearing grease nipple painted over- no sign of grease","Deck - Machinery,Miscellaneous","General Appearance","Equipment Related","","","","","All grease nipples made free of paint and properly lubricated","2019-01-23","","Completed","2019-01-23","No","No","No","Internal"]
[null,null,null,null,2384,"54_14/10/2019 5:38:05 AM","2019-01-18","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Fuel common rail end cover flange damaged","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","To raise Ro for new flange and replace and same raised","2019-02-17","DRED190006","Completed","2019-02-02","No","No","No","Internal"]
[null,null,null,null,2385,"54_14/10/2019 5:39:20 AM","2019-01-18","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","As per PAL AE Thrust beraing renewal routine is 32000 hrs, but during last decarb in Nov/2018 only condition checks carried out.To check as per makers reccommondation and correct as nessary in PAL.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","checked as per makers reccommondation and same existing in PAL.","2019-02-17","","Completed","2019-01-19","No","No","No","Internal"]
[null,null,null,null,2386,"54_14/10/2019 5:40:22 AM","2019-01-18","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","As per PAL AE Gudgeon pin renewal routine is 32000 hrs.To check as per makers reccommondation and correct as nessary in PAL","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","checked as per makers reccommondation and same existing in PAL.","2019-02-17","","Completed","2019-01-19","No","No","No","Internal"]
[null,null,null,null,595,"54_Thu Oct 10 2019 18:20:13 GMT+0000","2019-01-18","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Port side hyd motor reported knocking sound while paying out at low speed mode only","Deck - Mooring Machinery","Mooring","Equipment Related","","","","","Motor replaced with new spare and working satisfcatoory.(Job order no: V-DRED018689/19)","2019-02-02","","Completed","2019-02-03","No","No","No","Internal"]
[null,null,null,null,596,"54_Thu Oct 10 2019 18:24:02 GMT+0000","2019-01-18","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Fwd PV breaker  for WBTS – liquid level not visible","Deck - Machinery","Cargo / Ballast Systems","Equipment Related","","","","","Liquid topped to required level","2019-01-25","","Completed","2019-02-02","No","No","No","Internal"]
[null,null,null,null,598,"54_Thu Oct 10 2019 18:31:29 GMT+0000","2019-01-18","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","SMGO bunker line desser coupling leaking near stbd side manifold ","Deck - Pipe / Fittings","MARPOL Related","Equipment Related","","","","","Dismantled the coupling and renewed them.","2019-01-28","","Completed","2019-02-09","No","No","No","Internal"]
[null,null,null,null,599,"54_Thu Oct 10 2019 18:39:19 GMT+0000","2019-01-18","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","BWTS deck seal tank empty","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","BWTS to be started and checked every month, all associated equipment to be kept in ready condition","2019-01-25","","Completed","2019-02-10","No","No","No","Internal"]
[null,null,null,null,600,"54_Thu Oct 10 2019 18:45:09 GMT+0000","2019-01-18","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Observed mast riser stay wires rusted and devoid of grease","Inert Gas","General Appearance","Inappropriate Procedure","","","","","To ensure wires are sufficiently greased to avoid rust/damage","2019-02-15","","Completed","2019-02-26","No","No","No","Internal"]
[null,null,null,null,602,"54_Thu Oct 10 2019 18:50:46 GMT+0000","2019-01-18","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Remote hyd valve box on deck, hinge & supports rusted","Cargo Mach.","General Appearance","Equipment Related,Inappropriate Procedure","","","","","To derust and avoid wastage of steel","2019-03-15","","Completed","2019-03-21","No","No","No","Internal"]
[null,null,null,null,603,"54_Thu Oct 10 2019 18:53:37 GMT+0000","2019-01-18","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Coaming thinned down/wasted at one location","Miscellaneous","General Appearance","External Factors","","","","","Complete assembly to dismantle and to be repaired at ER w/shop","2019-03-31","","Completed","2019-04-23","No","No","No","Internal"]
[null,null,null,null,608,"54_Tue Dec 10 2019 14:22:36 GMT+0000","2019-01-18","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","No test bench onboard for PV valve – given the numerous no. of valves (including for Ballast tanks)","Deck - Pipe / Fittings","Cargo / Ballast Systems","External Factors","","","","","R.O raised and approved from vessel's end","2019-04-30","DRED1900059","Completed","2019-08-21","No","No","No","Internal"]
[null,null,null,null,609,"54_Sat Oct 12 2019 14:27:45 GMT+0000","2019-01-18","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Lubricator, mositure drain filter found fully wrapped with denzo tape – completely unware of function inside","Deck - Mooring Machinery","Mooring","Equipment Related","","","","","To remove denzo tape, ensure same is maintained in working condition. Same complied with.","2019-01-23","","Completed","2019-01-22","No","No","No","Internal"]
[null,null,null,null,2443,"54_14/10/2019 10:03:57 PM","2019-01-18","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","DK PIPE / FITGS\tCargo manifold platform Gratings rusted","Deck - Pipe / Fittings","General Appearance","External Factors","","","","","Port side manifold gratings is  hyblasted and cosmetic maintenance is completed.","2019-04-30","","Completed","2019-05-30","No","No","No","Internal"]
[null,null,null,null,2444,"54_14/10/2019 10:48:58 PM","2019-01-18","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Gun retaining springs missing on Foam monitors #3, #4, #5 ","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","Foam monitor missing springs renewed.","2019-03-30","DRED 190054","Completed","2019-05-30","No","No","No","Internal"]
[null,null,null,null,2473,"54_14/10/2019 11:59:51 PM","2019-01-18","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","No test bench onboard for PV valve – given the numerous no. of valves (including for Ballast tanks)","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","","","","","R.O raised and approved from vessel's end","2019-04-30","DRED190059","Completed","2019-08-21","No","No","No","Internal"]
[null,null,null,null,2438,"54_14/10/2019 09:52:48 PM","2019-02-02","Defect","Ship Staff","Ship Staff Insp.","Many cabins toilet overhead light fitting covers found missing or broken.","Elect. Mach. & Equip.","General Appearance","Equipment Related","","","","","Missing lights and covers replaced with new one.","2019-04-30","DRED 190057","Completed","2019-05-28","No","No","No","Internal"]
[null,null,null,null,2492,"54_16/10/2019 5:29:27 AM","2019-02-02","Defect","Ship Staff","Ship Staff Insp.","In Galley entrance 20 w tube light globe is having crack","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","Same renewed.","2019-04-30","DRED 190057","Completed","2019-05-28","No","No","No","Internal"]
[null,null,null,null,610,"54_Sat Oct 12 2019 14:36:09 GMT+0000","2019-02-05","Defect","Ship Staff","Ship Staff Insp.","FWD mast steering light 220 volt insulation showing 0.5 mega ohms","Documentation","Navigation","Equipment Related","","","","","Checked and found steeing light fitting had crack same renewed with new spare one checked insulation found 100 mega ohms","2019-02-15","","Completed","2019-02-08","No","No","No","Internal"]
[null,null,null,null,2388,"54_14/10/2019 5:50:23 AM","2019-02-09","Critical Equipment","Ship Staff","Ship Staff Insp.","Emergency geneartor, observed leakage from the radiator in the middle section of the unit.","E/R - Aux. Mach.","Emgcy. Systems","Equipment Related","","","","","Cold repair carrried out. PO raised in PAL DRED 190061.(Job order no: V-DRED018251/19)","2019-03-30","DRED 190061","Completed","2019-02-17","No","No","No","Internal"]
[null,null,null,null,2393,"54_14/10/2019 5:58:13 AM","2019-02-10","Defect","Ship Staff","Ship Staff Insp.","Deck seal pump#1 impeller key and shaft found damaged.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Requisition has been raised, for the time being shaft has been replaced with Ballast deck seal pump #2","2019-03-30","DRED 190065","Completed","2019-02-11","No","No","No","Internal"]
[null,null,null,null,613,"54_Tue Dec 10 2019 14:44:39 GMT+0000","2019-02-10","Defect","Ship Staff","Ship Staff Insp.","Deck seal pump#1 impeller key and shaft found damaged.","Deck - Machinery","Cargo / Ballast Systems","Equipment Related","","","","","Requisition has been raised. PO no DRED 190065. for the time being shaft has been replaced with Ballast deck seal pump #2","2019-03-30","DRED 190065","Completed","2019-02-11","No","No","No","Internal"]
[null,null,null,null,612,"54_Sat Oct 12 2019 14:41:41 GMT+0000","2019-02-11","Defect","Ship Staff","Ship Staff Insp.","During greasing and closeup inspection of mooring wires, found strands of aft spring mooring wire on drum MW6B, broken at ~15 mtrs from eye. Upon calculation of no. of strands broken, confirmed that this end of wire is unfit for use and requires to be changed End for End or Replaced. Note: As per available maintenance records, this mooring wire was turned end to end on 09 May 2017.","Deck - Mooring Machinery","Mooring","Equipment Related","","","","","Wire to be changed End for End or Replaced with spare mooring wire on board. Update as on 08 Mar 2019: Vessel has turned the wire End for End and this wire shall be replaced once New wire is received on board.","2019-03-15","","Completed","2019-03-08","No","No","No","Internal"]
[null,null,null,null,611,"54_Sat Oct 12 2019 14:38:42 GMT+0000","2019-02-12","Defect","Ship Staff","Ship Staff Insp.","Bridge stbd wing Anemometer display found fallen down ","Navigation - Others","Navigation","Equipment Related","","","","","Panel open removed Display unit and fitted back.(Job order no: V-DRED019407/19) ","2019-02-15","","Completed","2019-02-14","No","No","No","Internal"]
[null,null,null,null,2391,"54_14/10/2019 5:55:04 AM","2019-02-15","Defect","Ship Staff","Ship Staff Insp.","DG no.1 turbocharger cartridge found clogged with carbon deposit.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Same was removed and cleaned. Nozzle ring changed. DG tried out OK","2019-02-16","Job order no: V-DRED019408/19","Completed","2019-02-15","No","No","No","Internal"]
[null,null,null,null,614,"54_Sat Oct 12 2019 14:49:02 GMT+0000","2019-02-18","Defect","Ship Staff","Ship Staff Insp.","During GMDSS battery load test on 17.2.19 its found after 7 hrs battery voltage dropped bellow alarm level.","Navigation - GMDSS & Communication","Navigation","Equipment Related","","","","","Batteries rechanged and showing 25.7 volts. Batteries replaced with new one.","2019-04-30","DRED 190070","Completed","2019-04-21","No","No","No","Internal"]
[null,null,null,null,615,"54_Tue Dec 10 2019 16:08:19 GMT+0000","2019-02-18","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","During GMDSS battery load test on 17.2.19 its found after 7 hrs battery voltage dropped bellow alarm level. Batteries rechanged and showing 25.7 volts.","Navigation - GMDSS & Communication","Communication","Equipment Related","","","","","Batteries replaced with new one.","2019-04-29","DRED190050","Completed","2019-04-21","No","No","No","Internal"]
[null,null,null,null,2390,"54_14/10/2019 5:53:34 AM","2019-02-19","Defect","Ship Staff","Ship Staff Insp.","M/E unit no.1 exhaust valve fail and early closing alarm activating- frequently.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","FCM module ,exhaust valve replaced. Still Alarm triggering occasionaly. VCU changed .","2019-02-28","V-DRED000486/16","Completed","2019-02-22","No","No","No","Internal"]
[null,null,null,null,2389,"54_14/10/2019 5:52:15 AM","2019-02-20","Defect","Ship Staff","Ship Staff Insp.","Emergency Generator cooling water heater found not working.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","checked and found one terminal found burnt same renewed with new one tried out found satisfactory.(Job order no: V-DRED019141/19)","2019-02-22","V-DRED019141/19","Completed","2019-02-21","No","No","No","Internal"]
[null,null,null,null,2392,"54_14/10/2019 5:56:24 AM","2019-02-27","Defect","Ship Staff","Ship Staff Insp.","Waste water overboard line on stbd side has got a hole.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Need to fabricate new pipe. Currently cold repair has been carried out. Permanent repair will be carried out in Ballast passage","2019-03-27","","Completed","2019-03-05","No","No","No","Internal"]
[null,null,null,null,618,"54_Sat Oct 12 2019 16:32:28 GMT+0000","2019-03-18","Critical Equipment,Defect","Ship Staff","Ship Staff Insp.","SCBA Straps found Cracked.","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","Spares recd. And changed in Rizhao, CHINA.","2019-04-30","DRED190054","Completed","2019-04-05","No","No","No","Internal"]
[null,null,null,null,2394,"54_14/10/2019 6:00:56 AM","2019-03-21","Defect","Ship Staff","Ship Staff Insp.","220volts low insulation 1 mega ohms  on deck midship port flood light","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","Equipment Related","","","","","checked and found junction box some water ingressed found same cleaned and dryed treid out found insulation 80 mega ohms ","2019-03-24","","Completed","2019-03-22","No","No","No","Internal"]
[null,null,null,null,616,"54_Sat Oct 12 2019 16:16:42 GMT+0000","2019-03-21","Defect","Ship Staff","Ship Staff Insp.","220volts low insulation 1 mega ohms  on deck midship port flood light ","Deck - Pipe / Fittings,Elect. Mach. & Equip.","General Appearance","Equipment Related","","","","","checked and found junction box some water ingressed found same cleaned and dryed treid out found insulation 80 mega ohms","2019-03-24","","Completed","2019-03-22","No","No","No","Internal"]
[null,null,null,null,617,"54_Sat Oct 12 2019 16:19:27 GMT+0000","2019-03-25","Defect","Ship Staff","Ship Staff Insp.","Spilt bearing of Port windlass winch outboard drum gear shaft out of place.","Deck - Mooring Machinery","Mooring","Equipment Related","","","","","Split bearing renewed. Please refer job no. V-DRED020399/19 for further details.","2019-04-30","","Completed","2019-03-27","No","No","No","Internal"]
[null,null,null,null,619,"54_Sat Oct 12 2019 16:36:01 GMT+0000","2019-03-27","Defect","Ship Staff","Ship Staff Insp.","STBD cargo line No 1 manifold pressure showing 0 in CCR PMS display.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","","","","","Safty Barrier renewed with spare one raised.","2019-04-20","","Completed","2019-04-23","No","No","No","Internal"]
[null,null,null,null,2428,"54_14/10/2019 09:24:59 PM","2019-03-27","Defect","Ship Staff","Ship Staff Insp.","STBD cargo line No 1 manifold pressure showing 0 in CCR PMS display.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","Safty Barrier renewed with spare one raised.","2019-04-20","DRED190094","Completed","2019-04-23","No","No","No","Internal"]
[null,null,null,null,7446,"54_Sat Oct 12 2019 16:40:00 GMT+0000","2019-03-29","Defect","Ship Staff","Ship Staff Insp.","Ship side scupper on Port Lifeboat deck found choked.","Deck - Pipe / Fittings","General Appearance","Equipment Related","","","","","Vessel has tried clearing the scupper pipe by various means, viz. hammering of the scupper pipe inside port void space, hydro blasting into the scupper pipe to clear debris, snake wire, derust liquid, but nothing has been effective. Solution: To rig staging on the ship side and try to clear the horizontal choked section from ship side externally. Vessel shall try to undertake this job at a suitable and safe anchorage at next available opportunity. Since vessel unable to clear the choke, have raised REFMAN for carrying out the job during DD. Note: The length of the scupper pipe is almost 5 meters inside the void space and is without any flange.","2019-05-31","","Completed","2019-08-15","Yes","No","No","Internal"]
[null,null,null,null,2459,"54_14/10/2019 11:29:07 PM","2019-03-29","Defect","Ship Staff","Ship Staff Insp.","Ship side scupper on Port Lifeboat deck found choked.","Deck - Pipe / Fittings","General Appearance","Equipment Related","","","","","Vessel has tried clearing the scupper pipe by various means, viz. hammering of the scupper pipe inside port void space, hydro blasting into the scupper pipe to clear debris, snake wire, derust liquid, but nothing has been effective. Solution: To rig staging on the ship side and try to clear the horizontal choked section from ship side externally. Vessel shall try to undertake this job at a suitable and safe anchorage at next available opportunity. Since vessel unable to clear the choke, have raised REFMAN for carrying out the job during DD. Note: The length of the scupper pipe is almost 5 meters inside the void space and is without any flange.","2019-05-31","","Completed","2019-08-15","No","No","No","Internal"]
[null,null,null,null,2404,"54_14/10/2019 6:22:54 AM","2019-03-30","Defect","Ship Staff","Ship Staff Insp.","General service batteries loadtest found battery drop below level","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","Battery replaced with the newly received once.","2019-04-30","DRED190105","Completed","2019-04-21","No","No","No","Internal"]
[null,null,null,null,625,"54_Sat Oct 12 2019 16:58:12 GMT+0000","2019-04-06","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Recommend to fit quick release securing for embarkation ladders as currently the securing will take time to open","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","At present our embarkation ladder covers can be opened up by 2 persons within a minute. Hence the arrangement is found satisfactory from ship's end.","2019-04-15","","Completed","2019-04-08","No","No","No","Internal"]
[null,null,null,null,7474,"54_Tue Nov 12 2019 03:42:09 GMT+0000 (Coordinated Universal Time)","2019-04-07","Non Conformity","Owner / Marine / Tech. Suptd.","ISM Audit","Pump room bottom telephone cable protection seathing was observed to be cracked in few location","Navigation - GMDSS & Communication","Communication","Equipment Related","5.21","Medium","","","ETO replaced the pump room telephone head-set cable with the only one spare cable he had immediately. An order for a new spare has been made on the 09th April 2019.(DRED 190115)","2019-07-06","","Completed","2019-04-10","No","No","No","Internal"]
[null,null,null,null,7476,"54_Tue Nov 12 2019 03:48:04 GMT+0000 (Coordinated Universal Time)","2019-04-07","Defect","Owner / Marine / Tech. Suptd.","ISM Audit","2 nos chain block were observed with\n\nthe locking plate for hooks missing / not\n\nfunctioning correctly","Miscellaneous","General Appearance","Equipment Related","8.81","Low","","","DO NOT USE' tags were put on the chain blocks immediately.","2019-07-07","","Completed","2019-04-10","No","No","No","Internal"]
[null,null,null,null,7477,"54_Tue Nov 12 2019 04:01:16 GMT+0000 (Coordinated Universal Time)","2019-04-07","Defect","Owner / Marine / Tech. Suptd.","ISM Audit"," Item 3.2.3 of IOPP form-B mentions\n\n\"Residue(sludge) is transferred to slop tanks (s) in line with example#23 of MEPC.1/Circ.736\" as only other acceptable means for disposal of oil residues (sludge). However vessel is also using evaporation from 'FO Sludge storage tank' and\n\n'Incinerator waste oil tank' as means for disposal of oil residues (sludge).","E/R - Pipes/ valves & fittings","Cert. & Docu.","Industry Issue","6.5","Medium","","","Before using these tanks for evaporating request to include these tank in IOPP-form B should have been made so as to meet the regulation requirement. To check the certificates on joining for correctness of data in them.","2019-07-07","","Completed","2019-04-19","No","No","No","Internal"]
[null,null,null,null,7478,"54_Tue Nov 12 2019 04:42:33 GMT+0000 (Coordinated Universal Time)","2019-04-07","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Cargo Audit - Readings for midship draft guage stbd side in CCR found to be not matching with actual","Deck - Machinery","Cargo / Ballast Systems","Equipment Related","8.2","Medium","","","VESSEL RENEWED THE PCB OF THE STARBOARD SIDE DRAFT GUAGE AND NOW THE READING ARE MATCHING WITH THE ACTUAL DRAFT READING AS VERIFIED BY THE LOADICATOR.","2019-07-07","","Completed","2019-05-12","No","No","No","Internal"]
[null,null,null,null,7479,"54_Tue Nov 12 2019 04:46:16 GMT+0000 (Coordinated Universal Time)","2019-04-07","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Cargo Audit - Manifold 1s (Fwd) Pressure readout in CCR found not operational","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.2","Medium","","","VESSEL RENEWED THE ZENER BARRIER AND READINGS ARE NOW REPEATING IN THE REMOTE PRESSURE TRANSMITTOR.","2019-07-06","","Completed","2019-04-23","No","No","No","Internal"]
[null,null,null,null,7480,"54_Tue Nov 12 2019 04:53:44 GMT+0000 (Coordinated Universal Time)","2019-04-07","Defect","Owner / Marine / Tech. Suptd.","Nav Audit / Verification","Navtex printer is not printing proper on auto mode. Printout has be taken manually by pulling paper with hand. Requisition has been raised for same.","Navigation - GMDSS & Communication","Navigation","Equipment Related","4.1","High","","","The technician attended in Singapore and changed the Navtex unit and the new navtex unit is working satisfactorily","2019-07-06","","Completed","2019-04-18","No","No","No","Internal"]
[null,null,null,null,2395,"54_14/10/2019 6:08:46 AM","2019-04-07","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Tell-tale signs of leakage visible near FO sludge pump","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Area cleaned","2019-04-15","","Completed","2019-04-08","No","No","No","Internal"]
[null,null,null,null,2396,"54_14/10/2019 6:10:02 AM","2019-04-07","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","A/E-2 Duplex filter observed to have minor leakage","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","No leakage there. Area cleaned","2019-04-15","","Completed","2019-04-07","No","No","No","Internal"]
[null,null,null,null,2397,"54_14/10/2019 6:11:09 AM","2019-04-07","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Recommend to fit guard or warning around no-1,2,3 central cooling FW pump, COPT condenser SW pump","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","guards fabricated and put in place","2019-04-15","","Completed","2019-04-11","No","No","No","Internal"]
[null,null,null,null,2398,"54_14/10/2019 6:12:35 AM","2019-04-07","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Small Oil observed in bilge & adjoining pipe around No-2 main lub oil pump","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Area cleaned","2019-04-15","","Completed","2019-04-12","No","No","No","Internal"]
[null,null,null,null,2399,"54_14/10/2019 6:14:08 AM","2019-04-07","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Various laggings in purifier room having superficial damage giving poor impression","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Laggings changed","2019-04-20","","Completed","2019-04-14","No","No","No","Internal"]
[null,null,null,null,2400,"54_14/10/2019 6:16:05 AM","2019-04-07","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Focused cleaning required in purifier room as Tell-tale signs of previous leakages clearly visible","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Area  cleaned","2019-04-18","","Completed","2019-04-13","No","No","No","Internal"]
[null,null,null,null,2401,"54_14/10/2019 6:18:23 AM","2019-04-07","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","All 440v electrical starter panels to have “Electrical Hazar” IMO symbol. Same recommended for 220v as well","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","IMO symbols will be pasted","2019-04-30","","Completed","2019-04-14","No","No","No","Internal"]
[null,null,null,null,2402,"54_14/10/2019 6:19:42 AM","2019-04-07","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Buckle & Hooks for harness in engine room escape started to show signs of corrosion","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","Same attended to and closed out from vessel's end.","2019-04-25","","Completed","2019-04-13","No","No","No","Internal"]
[null,null,null,null,2403,"54_14/10/2019 6:21:16 AM","2019-04-07","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Headset for pump room top and bottom telephone was observed to be with broken cable","Navigation - GMDSS & Communication","Communication","Equipment Related","","","","","Headset cable of pump room top and bottom has been changed and a requisition raised for a spare headset","2019-04-30","DRED190115","Completed","2019-04-08","No","No","No","Internal"]
[null,null,null,null,622,"54_Sat Oct 12 2019 16:47:39 GMT+0000","2019-04-07","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Lowest pressure Alarm displayed on CCR pressure transmitter panel","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","After testing the alarms of the pressure transmitter, the alarms to be set to zero.","2019-04-10","","Completed","2019-04-09","No","No","No","Internal"]
[null,null,null,null,2417,"54_14/10/2019 8:24:21 PM","2019-04-07","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Colour coding of DCP fire extinguisher\tSUP\tVessel's fire extinguishers comply with the colour coding requirements(5% of total external area of the fire extinguisher body) as per Code of Safe working practices","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","Vessel has DCP extinguisher-Blue colour, CO2 extinguisher- Black colour and Foam extinguisher- Yellow colour.","2019-04-30","","Completed","2019-04-09","No","No","No","Internal"]
[null,null,null,null,626,"54_Sat Oct 12 2019 17:01:35 GMT+0000","2019-04-07","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Garden hose to be fitted below the ream of metal half drums kept at manifold to avoid metal to metal contacts","Miscellaneous","General Appearance","Behaviour Based,Industry Issue","","","","","Own ship places rubber insulation mats below the drums, which serve the purpose of preventing metal to metal contact. Rubber mats cut to ensure they don’t cover any excess area beyond the half drum to ensure that any seepage beyond the half drum will go in ","2019-04-15","","Completed","2019-04-08","No","No","No","Internal"]
[null,null,null,null,2418,"54_14/10/2019 8:33:39 PM","2019-04-07","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Few life buoy grabs life fitted are flat type thus less than 10mm on few locations","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","As per the LSA code, the grablines of the lifebuoys should be not less than 9.5mm. The ones which were of the flat type had the original grablines fitted on them and they were supplied as such onboard. The vessel has already renewed 2 nos. of lifebouys with grablines of more than 9.5mm. All lifebouys grablines comply with the LSA code at present","2019-04-12","","Completed","2019-04-10","No","No","No","Internal"]
[null,null,null,null,2419,"54_14/10/2019 8:40:13 PM","2019-04-07","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Abandon ship drill reports were observed to be copy paste from the previous one for the past 3 months","Documentation","Cert. & Docu.","Human Error","","","","","Timings being recorded as per the actual reporting during the drill.","2019-04-15","","Completed","2019-04-13","No","No","No","Internal"]
[null,null,null,null,2420,"54_14/10/2019 8:44:11 PM","2019-04-07","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Key log to be updated for current crew\t","Documentation","Cert. & Docu.","Inappropriate Procedure","","","","","Key log updated for current crew onboard","2019-04-25","","Completed","2019-04-10","No","No","No","Internal"]
[null,null,null,null,2421,"54_14/10/2019 8:48:02 PM","2019-04-07","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Anchor brake indicator washer not matching with the indicator plate fitted","Deck - Mooring Machinery","Mooring","Equipment Related","","","","","There is no anchor brake indicator washer present on the brake cylinders. When the anchor brake is tightened up, the brake cylinder shaft rises up from the cylinder and similarly when the brake is slackened, the brake cylinder shaft sets down towards the cylinder. Marking have been highlightened on the grooving of the brake cylinder shaft at the bottom of the brake cylinder and correspondingly on the indicator plate to confirm if the brake has been fully tightened or slackened.","2019-04-20","","Completed","2019-04-15","No","No","No","Internal"]
[null,null,null,null,2429,"54_14/10/2019 09:29:31 PM","2019-04-07","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Minor hydraulic leakage observed from control lever of Fwd breast mooring winch and Port windlass winch controller","Deck - Machinery","Mooring","Equipment Related","","","","","eak rectified by renweing the shaft seal and o' rings.","2019-04-30","","Completed","2019-05-30","No","No","No","Internal"]
[null,null,null,null,2445,"54_14/10/2019 10:55:06 PM","2019-04-07","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Minor hydraulic leakage observed from control lever of Fwd breast mooring winch and Port windlass winch controller+ aft mooring winch center","Deck - Mooring Machinery","Mooring","Equipment Related","","","","","Leak rectified by renweing the shaft seal and o' rings.","2019-04-30","","Completed","2019-05-30","No","No","No","Internal"]
[null,null,null,null,2447,"54_14/10/2019 10:59:49 PM","2019-04-07","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Fabrication of stand for mounting of light on stbd side forward for life raft","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","Stand fabricated and give to chief officer for installation.","2019-06-07","","Completed","2019-06-06","No","No","No","Internal"]
[null,null,null,null,2488,"54_16/10/2019 5:23:00 AM","2019-04-07","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Focused cleaning required on the aft part of AE-1,2,3","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","Aft side of DG Area cleaned.","2019-06-18","","Completed","2019-05-26","No","No","No","Internal"]
[null,null,null,null,2497,"54_16/10/2019 5:36:13 AM","2019-04-07","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Focused cleaning required on the aft part of main engine below common rail plug, near emergency manoeuvring area, on various electrical cables etc all having oil stains on it","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","Area on part of main engine below common rail plug, near emergency manoeuvring area,electrical cables etc all cleaned.","2019-06-25","","Completed","2019-06-08","No","No","No","Internal"]
[null,null,null,null,2409,"54_14/10/2019 6:32:03 AM","2019-04-15","Defect","Ship Staff","Ship Staff Insp.","Gen LO purifier non operational due to lack of spare.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Handle connection piece  replaced . Purifier made opeartional.","2019-04-30","DRED 190066","Completed","2019-04-21","No","No","No","Internal"]
[null,null,null,null,2523,"54_16/10/2019 6:35:16 AM","2019-04-16","Defect","Ship Staff","Ship Staff Insp.","Aux-Engine F.O  back wash filter digital differential pressure found defective","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Differential switch found defective no spare on board ","2019-07-30","DRED 190119","Completed","2019-08-30","No","No","No","Internal"]
[null,null,null,null,2410,"54_14/10/2019 6:34:01 AM","2019-04-18","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","E/R blower room ceiling lagging is coming out from some areas. Same needs to be secured.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","E/R blower room ceiling lagging secured.","2019-04-28","","Completed","2019-04-27","No","No","No","Internal"]
[null,null,null,null,2411,"54_14/10/2019 6:35:25 AM","2019-04-18","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Auto drain of all the air bottles are kept shut. As per fourth engineer same is kept shut because it is leaking. TO be overhauled and all the auto drains to be kept open.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Auto drain of all the air bottles  overhauled and all the auto drains kept open.","2019-05-18","","Completed","2019-04-24","No","No","No","Internal"]
[null,null,null,null,2412,"54_14/10/2019 6:36:43 AM","2019-04-18","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Boiler fuel pump no 2 found leaking from the seals. TO be overhauled.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","Leakage from the pump rectified by cleaning the oil seal.","2019-04-28","","Completed","2019-04-27","No","No","No","Internal"]
[null,null,null,null,2423,"54_14/10/2019 9:01:41 PM","2019-04-18","Defect","Ship Staff","Ship Staff Insp.","During GMDSS battery load test on 17.2.19 its found after 7 hrs battery voltage dropped bellow alarm level. Batteries rechanged and showing 25.7 volts.","Navigation - GMDSS & Communication","Navigation","Equipment Related","","","","","Batteries replaced with new one","2019-04-30","DRED 190070","Completed","2019-04-21","No","No","No","Internal"]
[null,null,null,null,2424,"54_14/10/2019 09:13:39 PM","2019-04-18","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Wooded plank of the some of the shelf in chemical locker needs to be renewed","Miscellaneous","General Appearance","Equipment Related","","","","","Wooden planks renewed.","2019-04-28","","Completed","2019-04-22","No","No","No","Internal"]
[null,null,null,null,2425,"54_14/10/2019 09:16:34 PM","2019-04-18","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","One of the container of chemical is fully corroded and can leak any time. Transfer the content to other container. Similarly to check all other old containers","Miscellaneous","General Appearance","Inappropriate Procedure","","","","","Rusted Chemical container content transferred to spare one.Rest all other container in good condition.\t28-Oct-19","2019-10-28","","Completed","2019-04-22","No","No","No","Internal"]
[null,null,null,null,2426,"54_14/10/2019 09:19:41 PM","2019-04-18","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Sound powered phone mouth piece at emergency maneuvering platform is damaged. Needs to be rectified/replaced.","Elect. Mach. & Equip.","Communication","Equipment Related","","","","","Sound power phone mouth piece replaced with the spare one.","2019-04-28","","Completed","2019-04-22","No","No","No","Internal"]
[null,null,null,null,2427,"54_14/10/2019 09:22:18 PM","2019-04-18","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","One of the Ref bottle is secured by rope. Permanent arrangement to make.","Miscellaneous","General Appearance","Inappropriate Procedure","","","","","Additional securing arrangements for the spare ref bottle made .","2019-04-28","","Completed","2019-04-22","No","No","No","Internal"]
[null,null,null,null,2442,"54_14/10/2019 10:01:01 PM","2019-04-18","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Emergency fire pump space bulkheads, light fittings needs cleaning. Pleanty dust were sighted. ","Miscellaneous","General Appearance","Inappropriate Procedure","","","","","Emergency fire pump space bulkheads, side stringers ,light fittings are and the floor cleanded.","2019-05-18","","Completed","2019-05-29","No","No","No","Internal"]
[null,null,null,null,2449,"54_14/10/2019 11:05:40 PM","2019-04-18","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Location of spares is not mentioned in PAL, Same to be entered properly.","Documentation","Cert. & Docu.","Inappropriate Procedure","","","","","Spares Updated in PAL.","2019-06-18","","Completed","2019-06-19","No","No","No","Internal"]
[null,null,null,null,2451,"54_14/10/2019 11:09:45 PM","2019-04-18","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Pump room area side structures needs to be cleaned off dust","Miscellaneous","General Appearance","External Factors","","","","","Same has been attended to when it is raining and will further cleaned during rains. Pumproom cleaning has been carried out and will be continued further as and when requiring attention","2019-07-18","","Completed","2019-06-25","No","No","No","Internal"]
[null,null,null,null,2474,"54_15/10/2019 12:02:38 AM","2019-04-18","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","\tPipe support structure on deck in aft area, needs to be derusted and painted.","Deck - Pipe / Fittings","General Appearance","External Factors","","","","","Same to be attended and closed out, once forward pipelines maintenance is completed.","2019-10-18","","Completed","2019-05-30","No","No","No","Internal"]
[null,null,null,null,2486,"54_16/10/2019 5:19:21 AM","2019-04-18","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Air found leaking from the air supply arrangement of ME top bracing. Same to be rectified.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Leak rectified by overhauling the reducing valve.","2019-04-28","","Completed","2019-05-17","No","No","No","Internal"]
[null,null,null,null,2489,"54_16/10/2019 5:25:39 AM","2019-04-18","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","All the fire alarm sensor are marked on floor by sticking laminated paper, which is not going to last. Same is true for all the fire sensor in engine room. All to be stenciled.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","All the fire alarm sensor stenciled in engine room.","2019-06-18","","Completed","2019-05-27","No","No","No","Internal"]
[null,null,null,null,2490,"54_16/10/2019 5:26:47 AM","2019-04-18","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","DG Area side side structure needs to be cleaned as same covered with dust . Laggings around DG area also needs external cleaning. ( pic attached).","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","DG Area side side structure cleaned . Laggings around DG area cleaned and painted.","2019-06-18","","Completed","2019-05-17","No","No","No","Internal"]
[null,null,null,null,2491,"54_16/10/2019 5:28:09 AM","2019-04-18","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Big motor body fins needs to be cleaned. (pic attached)","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","Main Big motors fins cleaned an some minor motors in progress and in continuation the job will be attended on regular basis.","2019-06-18","","Completed","2019-05-25","No","No","No","Internal"]
[null,null,null,null,2493,"54_16/10/2019 5:31:13 AM","2019-04-18","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Air duct in BWTS area and near boiler platform port side is badly corroded. Needs to do some repair. Include same in Refman as well if can't repair","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Same patched up and painted.","2019-06-18","","Completed","2019-05-31","No","No","No","Internal"]
[null,null,null,null,2498,"54_16/10/2019 5:37:35 AM","2019-04-18","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Some soft patched on the flocculation tank of OWS needs to be repaired.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","Cold repair carried out. Same holding good.","2019-05-18","","Completed","2019-06-06","No","No","No","Internal"]
[null,null,null,null,2500,"54_16/10/2019 5:39:56 AM","2019-04-18","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Various light fittings in E/R needs to be cleaned as same is covered with dust. ( Pic Attached)","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","Light fitting clenaing done.","2019-06-18","","Completed","2019-06-10","No","No","No","Internal"]
[null,null,null,null,2504,"54_16/10/2019 5:45:18 AM","2019-04-18","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","T/C air intake room is very much ignored. All fittings are rusted and area is very dirty. Proper maintanace needs to be carried out. The door for this room is very hard to operate. To free up and grease. ( Pic Attached)","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","T/C air intake room fittings etc cleaning done. Door has been freed.","2019-06-30","","Completed","2019-06-29","No","No","No","Internal"]
[null,null,null,null,2414,"54_14/10/2019 6:39:23 AM","2019-04-24","Defect","Ship Staff","Ship Staff Insp.","ME sump oil contaning about 1.25% water as per shore analysis report","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Purification of the oil completed .Continous purification of the oil in progress. Present lube oil test showing water 0.02%.","2019-05-15","","Completed","2019-05-07","No","No","No","Internal"]
[null,null,null,null,2415,"54_14/10/2019 6:40:34 AM","2019-04-24","Defect","Ship Staff","Ship Staff Insp.","TG lube oil as per shore analysis showing water content 0.25%","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Purification of the oil completed .Present lube oil test showing water %0.02%.","2019-05-31","","Completed","2019-05-12","No","No","No","Internal"]
[null,null,null,null,2487,"54_16/10/2019 5:20:46 AM","2019-04-24","Defect","Ship Staff","Ship Staff Insp.","TOP bracing no. 1 fwd to be checked for slight oil leakage from the seal rings of the indicator.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Seal ring of top brazing indicator for no. 1 and 2 renewed. Same OK and no leak.","2019-06-24","","Completed","2019-05-27","No","No","No","Internal"]
[null,null,null,null,2406,"54_14/10/2019 6:25:52 AM","2019-04-27","Defect","Ship Staff","Ship Staff Insp.","ME LO purifier found making abnormal noise during operation","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","After dismantling the purifier, observed that the spindle on way of bearing seat area eroded by about 2 mm and the bearing was loose on shaft. The direction of the assembling angular contact bearing for one no was wrong also The bearing sleeve was worn out. Vetical shaft and all bearings replaced and boxed back and tried out now working satisfactory.","2019-04-27","","Completed","2019-04-27","No","No","No","Internal"]
[null,null,null,null,2413,"54_14/10/2019 6:37:58 AM","2019-04-27","Defect","Ship Staff","Ship Staff Insp.","Air lock in cooling FW system. No.1 main air compressor was the source.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","After isolating the compressor complete overhauling of the compressor carried out. Suspected gasket renewed. Compressor tried out and working satisfactory.","2019-04-28","","Completed","2019-04-27","No","No","No","Internal"]
[null,null,null,null,2407,"54_14/10/2019 6:28:47 AM","2019-04-28","Defect","Ship Staff","Ship Staff Insp.","No.1 HFO purifier motor  tripping on high current","E/R - Purifier","Eng. / Strg. Comp.","Equipment Related","","","","","Motor coupling hub bearing dismantled and found 1 bearing no good, dismantled and replace all bearing and tried out now working satisfactory","2019-04-28","","Completed","2019-04-28","No","No","No","Internal"]
[null,null,null,null,2408,"54_14/10/2019 6:30:52 AM","2019-04-28","","Ship Staff","Ship Staff Insp.","No.2 HFO purifier during starting observed abnormal noise on the motor side and  high amperes","E/R - Purifier","Eng. / Strg. Comp.","Equipment Related","","","","","Motor coupling hub bearing dismantled and found seems to be okay and motor NDE and DE bearing inspected found DE bearing no good  dismantled and replace all bearing  and tried out now working satisfactory ","2019-04-28","DRED190123","Completed","2019-04-28","No","No","No","Internal"]
[null,null,null,null,2475,"54_16/10/2019 5:03:25 AM","2019-04-28","Defect","Ship Staff","Ship Staff Insp.","Water in oil detector sensor on BWMS found showing  1.0, same to be confirmed.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","Water in oil detector sensor on BWMS, same dismantled and cleaned. As there is no span 0 setting to set back in zero calibration. Actual water level was more then 0.9% ,same reduced to 0.02% by purification and presently its showing 0.29%.Pls note in clean oil sample the sensor was showing 0.56% watter content.","2019-05-15","","Completed","2019-05-07","No","No","No","Internal"]
[null,null,null,null,2503,"54_16/10/2019 5:43:42 AM","2019-04-29","Defect","Ship Staff","Ship Staff Insp.","ME Aux blower no.2 not starting in auto","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","Renewed A-4 control Relay contactor in  No-1 & 2 M/E Aux blower starter panel.","2019-06-16","","Completed","2019-06-29","No","No","No","Internal"]
[null,null,null,null,2416,"54_14/10/2019 6:41:54 AM","2019-04-30","Defect","Ship Staff","Ship Staff Insp.","Turning gear not working on remote  control.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","Trouble shooting completed and fault rectified in the lower connection point.","2019-05-15","","Completed","2019-05-05","No","No","No","Internal"]
[null,null,null,null,2405,"54_14/10/2019 6:24:30 AM","2019-05-02","Critical Equipment","Ship Staff","Ship Staff Insp.","Emergency generator, observed leakage from the radiator in the middle section of the unit.","Critical Equip.","Emgcy. Systems","Equipment Related","","","","","Old cold repaired radiator dismatled and replaced with new spare. Tried out and found working satisfactory and no sign of leakage.","2019-05-02","","Completed","2019-05-02","No","No","No","Internal"]
[null,null,null,null,2484,"54_16/10/2019 5:16:57 AM","2019-05-02","Defect","Ship Staff","Ship Staff Insp.","No.2 unit piston cooling oil outlet temp sensor showing erratic reading sometime, same to be checked.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","Connections checked and same tightened.","2019-06-15","","Completed","2019-05-21","No","No","No","Internal"]
[null,null,null,null,2485,"54_16/10/2019 5:17:52 AM","2019-05-02","Defect","Ship Staff","Ship Staff Insp.","NO.1 TG condensate pump not starting from remote in AMS panel.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","Same fault rectified and now able to start from AMS.","2019-06-02","","Completed","2019-05-26","No","No","No","Internal"]
[null,null,null,null,2507,"54_16/10/2019 5:48:46 AM","2019-05-06","Defect","Ship Staff","Ship Staff Insp.","EGB MIMIC  on AMS panel showing ME Stopped alarm and same not resetting. Same to be investigated.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Renewed A-4 control Relay contactor in  No-1 & 2 M/E Aux blower starter panel. Now no more alarm on panel. Same will be confirmed in passage.","2019-07-06","","Completed","2019-06-29","No","No","No","Internal"]
[null,null,null,null,2439,"54_14/10/2019 09:54:39 PM","2019-05-08","Defect","Ship Staff","Ship Staff Insp.","1P WBT sounding showing erratic reading of 1 meter","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","Sensor voltage checked and found 5V DC and input to PCB was 19.3V, output signal was 4.3mA. Zero adjustment carried out. Reading found to be around 30-35cm. Will observe during ballasting operations if it is showing correct reading or else will need to order a new PCB.","2019-05-30","","Completed","2019-05-20","No","No","No","Internal"]
[null,null,null,null,2476,"54_16/10/2019 5:04:31 AM","2019-05-08","Defect","Ship Staff","Ship Staff Insp.","ME Preheater for jacket cooling water inlet-outlet  valves leaking from joint. Same to be repaired. ","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","After isolation ME in STOP condition , flange gaskets for both the valves and bonnet gasket renewed.","2019-06-20","","Completed","2019-05-14","No","No","No","Internal"]
[null,null,null,null,2479,"54_16/10/2019 5:09:04 AM","2019-05-09","Defect","Ship Staff","Ship Staff Insp.","NO.1, 8,9 OMD sensor giving alarm, same to be checked.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","All connections checked and tigtened and presently no alarm for last 24 hrs.","2019-05-15","","Completed","2019-05-16","No","No","No","Internal"]
[null,null,null,null,2477,"54_16/10/2019 5:05:39 AM","2019-05-10","Defect","Ship Staff","Ship Staff Insp.","TBD boiler secondary master stop valve leaking from bonnet. Gasket to renew.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","After isolation, valve bonnet gasker renewed with metaflex gasket.","2019-05-25","","Completed","2019-05-15","No","No","No","Internal"]
[null,null,null,null,2430,"54_14/10/2019 09:32:03 PM","2019-05-11","Defect","Ship Staff","Ship Staff Insp.","For port life boat ,.F.O. retrurn pipe to fuel oil tank cracked ,same to be rectified by replacing.","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","Fuel oil return pipe leak rectified.","2019-05-13","","Completed","2019-05-12","No","No","No","Internal"]
[null,null,null,null,2431,"54_14/10/2019 09:34:21 PM","2019-05-11","Defect","Ship Staff","Ship Staff Insp.","For port side life boat, STBD battery to be checked and charging for same to be checked as same not able to start engine","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","For port side lifeboat both batteries renewed with spare one as they were due for replacement. Same working good after the changing and tried out.","2019-05-13","","Completed","2019-05-12","No","No","No","Internal"]
[null,null,null,null,2448,"54_14/10/2019 11:02:34 PM","2019-05-12","Defect","Ship Staff","Ship Staff Insp.","4nos. PV valves having slight leakages from the pressure side.(1C, 1S, 3P and SLP P COT)","Inert Gas","Cargo / Ballast Systems","Equipment Related","","","","","\tSLP P  and 3 P PV valve pressure side overhauled and leakages arrested. Others leakages very minor and being attended to.","2019-06-25","","Completed","2019-06-09","No","No","No","Internal"]
[null,null,null,null,2483,"54_16/10/2019 5:15:42 AM","2019-05-12","Defect","Ship Staff","Ship Staff Insp.","Air cooler drain for DG pipeline choke ,same to be cleared.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Air cooler drain line sections removed  and same cleared for all three DGS.","2019-05-20","","Completed","2019-05-25","No","No","No","Internal"]
[null,null,null,null,2433,"54_14/10/2019 09:38:37 PM","2019-05-13","Defect","Ship Staff","Ship Staff Insp.","DK MCRY\tPORT & STBD provision cranes, hoisting limit swtich non operational.","Deck - Machinery","General Appearance","Equipment Related","","","","","STBD provison crane hoisting limit system, driving shaft pin found sheared off due to siezed cam follower on the dhaft,same replaced with new pincam follower freed. Limits set and working satisfatory.For PORT provison crane also hoisting limit system, driving shaft pin found sheared off due to siezed brg .Cam follower also freed.same replaced with new pin. Limits set and working satisfatory","2019-05-20","","Completed","2019-05-18","No","No","No","Internal"]
[null,null,null,null,2478,"54_16/10/2019 5:07:38 AM","2019-05-15","Defect","Ship Staff","Ship Staff Insp.","Emergency DG spring starter input adaptor shaft cover slight crack noticed, same to be repaired by welding.","E/R - Aux. Mach.","Emgcy. Systems","Equipment Related","","","","","Same rectified by welding and fitted in place.","2019-05-17","","Completed","2019-05-16","No","No","No","Internal"]
[null,null,null,null,2499,"54_16/10/2019 5:38:51 AM","2019-05-15","Defect","Ship Staff","Ship Staff Insp.","ME Fuel rail steam tracing line ,flange gasket to renew.\t","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","flange gasket to renewed.","2019-06-15","","Completed","2019-06-10","No","No","No","Internal"]
[null,null,null,null,2506,"54_16/10/2019 5:47:34 AM","2019-05-15","Defect","Ship Staff","Ship Staff Insp.","440 volts low level insulation  Alarm  to be investigated and rectified.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","Renewed all 4 hot plate Element , no more 440 v low insulation from galley hot plate.","2019-06-20","","Completed","2019-06-23","No","No","No","Internal"]
[null,null,null,null,2432,"54_14/10/2019 09:36:00 PM","2019-05-16","Defect","Ship Staff","Ship Staff Insp.","Provision refer chambers -Fish room evaporator unit fan found making noise.","Miscellaneous","General Appearance","Equipment Related","","","","","Fan motor replaced with the spare motor  and working satisfactory.Old motor will be overhauled and kept as spare.","2019-05-17","","Completed","2019-05-17","No","No","No","Internal"]
[null,null,null,null,2482,"54_16/10/2019 5:14:20 AM","2019-05-18","Defect","Ship Staff","Ship Staff Insp.","No.1 Main air compressor brakdown. ( Con rod for HP side+HP piston+HP cylinder housing damaged)","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Compressor assembled back with avilable spares on board.Tried out and working satisfactory.","2019-05-28","","Completed","2019-05-26","No","No","No","Internal"]
[null,null,null,null,2434,"54_14/10/2019 09:41:21 PM","2019-05-19","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Portable extinguisher in fore peak store is obstructed with discarded rope. Same to be cleared off. ","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","Same cleared off","2019-05-29","","Completed","2019-05-21","No","No","No","Internal"]
[null,null,null,null,2436,"54_14/10/2019 09:46:28 PM","2019-05-19","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Steering Gear room Stbd bilge is obstructed with oil drums. Both bilge to be cleared and to be highlighted.","Miscellaneous","Eng. / Strg. Comp.","Inappropriate Procedure","","","","","Both bilge area cleared  highlighted.","2019-05-29","","Completed","2019-05-21","No","No","No","Internal"]
[null,null,null,null,2440,"54_14/10/2019 09:56:47 PM","2019-05-19","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Spider coupling of hydraulic pumps were found damaged in last inspection. Same has not been renewed yet.","Deck - Mooring Machinery","Mooring","Equipment Related","","","","","Spider coupling of all hydraulic pumps( Fwd 3 nos and Aft 3 Nos)  for mooring and windlass system, were found damaged and same replaced with new one. Motor tried out working satisfactory.","2019-06-19","","Completed","2019-05-29","No","No","No","Internal"]
[null,null,null,null,2441,"54_14/10/2019 09:58:54 PM","2019-05-19","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Air is leaking from test valve of stbd funnel flap. Same to be rectified.","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","Valve overhauled and leakage rectified.","2019-06-04","","Completed","2019-05-31","No","No","No","Internal"]
[null,null,null,null,2453,"54_14/10/2019 11:14:35 PM","2019-05-19","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Forward hydraulics starter panel is covered with canvas. Proper curtain arrangement to be made","Deck - Mooring Machinery","Mooring","Equipment Related","","","","","Proper curtain arrangement has been made for forward hydraulics panel.","2019-07-19","","Completed","2019-07-19","No","No","No","Internal"]
[null,null,null,null,2454,"54_14/10/2019 11:17:01 PM","2019-05-19","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","DK MCRY\tGreasing point of winches, weather tight doors and cranes to be marked with yellow for easy identification.","Deck - Machinery","General Appearance","Equipment Related","","","","","Highlighted all greasing points.","2019-07-19","","Completed","2019-07-15","No","No","No","Internal"]
[null,null,null,null,2455,"54_14/10/2019 11:19:16 PM","2019-05-19","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","AUS vacuum gauge seems not working,","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","same checked with pressure calibrator and working good.","2019-06-03","","Completed","2019-06-12","No","No","No","Internal"]
[null,null,null,null,2456,"54_14/10/2019 11:21:26 PM","2019-05-19","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","All the relief valve of the winches gear case are faulty. To be ordered or fabricated springs to be fitted.","Deck - Mooring Machinery","Mooring","Equipment Related","","","","","New springs fitted on the relief valves of the winches gear case.","2019-07-19","","Completed","2019-07-22","No","No","No","Internal"]
[null,null,null,null,2480,"54_16/10/2019 5:11:23 AM","2019-05-19","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Emergency fire pump space spring loaded valve is jammed, to be made free.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","SAME OPENED UP AND MADE FREE","2019-06-04","","Completed","2019-05-21","No","No","No","Internal"]
[null,null,null,null,2481,"54_16/10/2019 5:12:59 AM","2019-05-19","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Steering Gear drain pot behind DG area is clogged, to clear.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","Same made clear and free.","2019-05-29","","Completed","2019-05-21","No","No","No","Internal"]
[null,null,null,null,2494,"54_16/10/2019 5:32:30 AM","2019-05-27","Defect","Ship Staff","Ship Staff Insp.","ACONIS Procesor cabinet exhaust fan not working as motor windings showing open.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","Aconis Procesor cabinet exhaust fabrication of arrangements for fitting different size of cooling fan completed. Fitted with new fan (2 Nos) and tried out found satisfactory.","2019-06-27","","Completed","2019-05-31","No","No","No","Internal"]
[null,null,null,null,2501,"54_16/10/2019 5:41:06 AM","2019-06-02","Defect","Ship Staff","Ship Staff Insp.","For ER oil mist detection system , sensor fault for no. 2 unit ME area showing fault F1. Same to checked and rectified.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","Fault traced to be the cable for the sensor and same rectified.","2019-06-07","","Completed","2019-06-04","No","No","No","Internal"]
[null,null,null,null,2450,"54_14/10/2019 11:07:36 PM","2019-06-03","Defect","Ship Staff","Ship Staff Insp.","PORT side lifeboat, sprinkler pump spider coupling observed damaged, same to be repaired.","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","Coupling fabricated with the teflon rod and same fitted , tried out working good","2019-06-05","","Completed","2019-06-04","No","No","No","Internal"]
[null,null,null,null,2446,"54_14/10/2019 10:57:06 PM","2019-06-10","Defect","Ship Staff","Ship Staff Insp.","Forward mast one flood light not working\t","Miscellaneous","General Appearance","Equipment Related","","","","","Forward mast one flood light same checked, replaced bulb found still not working , replaced ballast transformer as well as capacitor  found still not working, rreplaced Igniter in terminal box of light found light working  RO for used spare will be raised","2019-06-12","","Completed","2019-06-12","No","No","No","Internal"]
[null,null,null,null,7470,"54_Sat Oct 12 2019 06:00:15 GMT+0000 (Coordinated Universal Time)","2019-06-12","Defect","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","Fixed Gas Detection System. THe sampling for the below areas were Observed disconnected.- Internal Sampling Point, Void Space, Bosun Store, Fore Peak Tnaks (which was found empty. Disconnected points were immediately activated by Chief Officer.","Miscellaneous","Cargo / Ballast Systems","Human Error","5.21","Medium","","","Senior officer is to physically check the condition of the gas detection system sampling points and to ensure that the sampling points which are to be kept connected are done so, so as to  avoid the system being in idle condition.","2019-06-18","","Completed","2019-06-12","No","No","No","External"]
[null,null,null,null,7471,"54_Sat Oct 12 2019 06:06:46 GMT+0000 (Coordinated Universal Time)","2019-06-12","Defect","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","Visitor Card. The safety contents sighted on the back were not legible(niether by the inspector nor the ship's staff). The same issue was observed in approx. 50% of the total Visitor's cards. Issue rectified before the inspector left the vessel ","Miscellaneous","ISPS Related","Inappropriate Procedure","5.12","Medium","","","All the visitor cards onboard are to be routinely checked for any smudged and illegible instructions on them to identify any deficiencies and rectify them promptly.\n\n\n\nSenior officer to routinely check the condition of the visitor cards and verify that they are in good order and properly legible. Deck officer is to verify the same prior to handing over the cards to the visitor.\n\n","2019-06-18","","Completed","2019-06-12","No","No","No","External"]
[null,null,null,null,7472,"54_Sat Oct 12 2019 06:12:14 GMT+0000 (Coordinated Universal Time)","2019-06-12","Defect","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","Winch Brake Test electronic format issued on March 2019 was sighted not in accordance with the MEG-4guidlines","Deck - Machinery","Mooring","Inappropriate Procedure","9.7","Medium","","","The format of the winch brake testing is to be based on the MEG-4 guidelines. Senior officers are to ensure that the same is being complied onboard.\n\n","2019-06-18","","Completed","2019-06-18","No","No","No","External"]
[null,null,null,null,7473,"54_Sat Oct 12 2019 06:17:20 GMT+0000 (Coordinated Universal Time)","2019-06-12","Defect","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","The ship desing MBL was observed described on the Mooring System Management Plan as 115.0T. Mooring Lines LDBF and TDBF were not known at the time of the inspection.","Miscellaneous","Mooring","Industry Issue","9.5","High","","","The LDBF and TDBF values of the mooring lines should be available as required by the MEG-4 guidelines. Correspondence with the manufacturer’s to be untaken and the values obtained to ensure compliance as the details are not known.\n\n","2019-06-18","","Completed","2019-06-18","No","No","No","External"]
[null,null,null,null,2502,"54_16/10/2019 5:42:33 AM","2019-06-12","Defect","Ship Staff","Ship Staff Insp.","One of the electrical panel for the DP transmitter on ME lube oil auto back wash filter not ptotected against accidental leak or spray from fire hydrants next to unit. ","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Safe guard for accidental spray provided in case the hydrant leaks for the electrical panel for the DP transmitter on ME lube oil auto back wash filter.","2019-06-12","","Completed","2019-06-12","No","No","No","Internal"]
[null,null,null,null,2505,"54_16/10/2019 5:46:24 AM","2019-06-12","Defect","Ship Staff","Ship Staff Insp.","L7 panel for fwd lighting group, showing low insulation even after switching off all the breakers in circuit.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","Renewed SBAG-202-N, No more low insulation alarm in L-7 Panel ","2019-06-20","","Completed","2019-06-24","No","No","No","Internal"]
[null,null,null,null,2495,"54_16/10/2019 5:34:13 AM","2019-06-13","Defect","Ship Staff","Ship Staff Insp.","No.2 AC compressor found V-belt axial play is more and one belts out of place. To check/replace","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","No.2 AC compressor v-belts found loose and axial play is more, same checked and replaced with new spare belts. Re-aligned and tried out found satisfactorily.","2019-06-14","","Completed","2019-06-13","No","No","No","Internal"]
[null,null,null,null,2496,"54_16/10/2019 5:35:16 AM","2019-06-13","Defect","Ship Staff","Ship Staff Insp.","ME LO Auto backwash filter body packing holder found slightly leaking to check/rectify","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","ME LO Auto backwash filter body paking holder found slightly leaking same checked and replaced x-ring 2 nos. Boxed back tested no leak.","2019-07-14","","Completed","2019-06-13","No","No","No","Internal"]
[null,null,null,null,7481,"54_Tue Nov 12 2019 04:59:26 GMT+0000 (Coordinated Universal Time)","2019-06-16","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Manifold pressure remote read out\n\nfor manifold in CCR found to be erratic","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.2","Medium","","","Zero calibration for STBD No-3 Aft  and  PORT No-2 Mid pressure transmitter was carried out and values adjusted accordingly, presently all transmitter are working satisfactorily.","2019-09-09","","Completed","2019-07-27","No","No","No","Internal"]
[null,null,null,null,7483,"54_Tue Nov 12 2019 05:08:11 GMT+0000 (Coordinated Universal Time)","2019-06-16","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Oxygen readings for ballast and\n\nvoid space in fixed gas detection system were observed to be incorrect","Miscellaneous","Cargo / Ballast Systems","Equipment Related","5.25","Medium","","","oil tankers of 20,000 tonnes deadweight and above, constructed on or after 1 January 2012, shall be provided with a fixed hydrocarbon gas detection system complying with the Fire Safety Systems Code for measuring hydrocarbon gas concentrations in all ballast tanks and void spaces of double-hull and double-bottom spaces adjacent to the cargo tanks, including the forepeak tank and any other tanks and spaces under the bulkhead deck adjacent to cargo tanks.\n\nThe regulation doesnot require to monitor oxygen in the ballast tank & void space","2019-09-09","","Completed","2019-06-20","No","No","No","Internal"]
[null,null,null,null,2513,"54_16/10/2019 6:17:35 AM","2019-06-18","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","No Oil max filters installed","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Installation of oil max filters completed.Only electrical breaker to be installed after receiving them.","2019-06-30","DRED 195010","Completed","2019-07-04","No","No","No","Internal"]
[null,null,null,null,2526,"54_16/10/2019 6:39:21 AM","2019-06-18","Defect","Owner / Marine / Tech. Suptd.","Ship Staff Insp.","E/R blower suction grid is damaged at various places. Replace the damaged grids.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","Received spares at singapore on 22nd August 2019 and same completed and damaged portion repaired.","2019-09-18","","Completed","2019-09-12","No","No","No","Internal"]
[null,null,null,null,2452,"54_14/10/2019 11:12:25 PM","2019-06-27","Defect","Ship Staff","Ship Staff Insp.","Galley starboard drain line pipe near overboard valve observe pin hole to be repair","E/R - Pipes/ valves & fittings","General Appearance","External Factors","","","","","Galley drain pipe same dismantled and renewed with new pipe","2019-07-05","","Completed","2019-07-01","No","No","No","Internal"]
[null,null,null,null,2508,"54_16/10/2019 5:49:55 AM","2019-06-28","Defect","Ship Staff","Ship Staff Insp.","No.1 AC compressor not loading more the single stage. Solenoid and loading mechanism to be checked and confirmed.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","No.1 AC compressor dismantled and found 2nd stage unloader(Fwd Stbd roller guide revit got sheared off) and 3rd stage unloader(Aft port roller guide revit  and plate where is the spring secured got sheared off also) same dismantled all piston and liner to have access for removing the unloading mechanism. Same replaced with new spare and boxed back. Aft stbd and port discharge valve new valve plate installed and suction valve for Aft port found 2 plate brokened same renewed with new spare. Top stbd suction valve plate also renewed. FWD port and Aft Stb conrod bearing checked and found having scoring marks same replaced with new spare. All crankcase door gasket renewed with new spare. Oil reflenished with fresh oil about 15ltrs. Boxed back and kept on standby.","2019-07-15","","Completed","2019-06-28","No","No","No","Internal"]
[null,null,null,null,2509,"54_16/10/2019 5:51:06 AM","2019-07-01","Defect","Ship Staff","Ship Staff Insp.","ME jacket pre-heater HT side gasket leaking gasket to be rene. ","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","ME jacket pre-heater HT side opened and same gasket replaced with new one.\t","2019-07-07","","Completed","2019-07-06","No","No","No","Internal"]
[null,null,null,null,2510,"54_16/10/2019 5:52:28 AM","2019-07-04","Defect","Ship Staff","Ship Staff Insp.","No.1 and 2 HP cicrculating pump outlet valve gland packing leaking. To be rectify","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","Both HP discharge valve bonnet gasket and gland packing renewed with new one","2019-07-07","","Completed","2019-07-06","No","No","No","Internal"]
[null,null,null,null,2511,"54_16/10/2019 5:53:35 AM","2019-07-07","Defect","Ship Staff","Ship Staff Insp.","During Running of no 2 D/G found tappet noise coming from no 6 unit . D/G immediately stopped and found one of the exhaust valve stuck in open position in valve guide.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Cylinder head dismantled and replaced with overhauled spare (complete cylinder head). All o-ring and gasket replaced with new one.","2019-07-07","","Completed","2019-07-07","No","No","No","Internal"]
[null,null,null,null,2466,"54_14/10/2019 11:44:48 PM","2019-07-12","Defect","Ship Staff","Ship Staff Insp.","Bridge A.C. not properly functioning","Elect. Mach. & Equip.","General Appearance","Equipment Related","","","","","condensor fan breaker coil internally shot and same replaced also found HP switch giving open signal and HP switch replaced with spare onboard","2019-08-20","","Completed","2019-08-29","No","No","No","Internal"]
[null,null,null,null,2512,"54_16/10/2019 6:16:00 AM","2019-07-22","Defect","Ship Staff","Ship Staff Insp.","M/E exhaust pipe funnel top Sway support upper side of welded area found wasted on both forward port and stbd support. Need to be attended and repaired by hot work.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","Welding of crack on the top of sway support was carried out. Two extra plates welded on both sides of the cracked sway plate for additional support. Also, on top of one the crack the doubler has been installed.","2019-07-26","","Completed","2019-07-26","No","No","No","Internal"]
[null,null,null,null,2514,"54_16/10/2019 6:18:43 AM","2019-07-22","Defect","Ship Staff","Ship Staff Insp.","ME rail unit starboard forward support on no.7 found crack elongated, need to be repair in DD.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","End of the crack which is still intact  drilled a hole to avoid extending of crack. Permanent repair method for same has to be worked out during  dry dock.Job included in RAFMAN.","2019-08-15","","Completed","2019-07-23","No","No","No","Internal"]
[null,null,null,null,2463,"54_14/10/2019 11:37:58 PM","2019-08-01","Defect","Ship Staff","Ship Staff Insp.","Pressure monitoring system of cargo manifold showing wrong reading in CCR","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","Trouble shooting in progress. Pressure calibration carried out and confirmed that port side pressure readings are matching with the CCR readout","2019-08-26","","Completed","2019-08-15","No","No","No","Internal"]
[null,null,null,null,2534,"54_17/10/2019 12:58:05 PM","2019-08-01","Defect","Ship Staff","Ship Staff Insp.","WBT soundings of 1S not showing correct reading.","Cargo Mach.,Hull & Tanks","Cargo / Ballast Systems","Equipment Related","8.12","Medium","","","Faulty sensor replaced with new sensor for sounding of 1S WBT. ","2019-11-20","","Completed","2019-12-10","No","No","No","Internal","RO no given is wrong. Please correct. DRED190149 is for Air con."]
[null,null,null,null,2458,"54_14/10/2019 11:26:30 PM","2019-08-04","Defect","Ship Staff","Ship Staff Insp.","Air is leaking from test valve of port bottom funnel flap. Same to be rectified.","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","Valve overhauled and leakage rectified.","2019-08-06","","Completed","2019-08-05","No","No","No","Internal"]
[null,null,null,null,2533,"54_17/10/2019 12:52:07 PM","2019-08-04","Defect","Ship Staff","Ship Staff Insp.","No.1 AC compressor discharge valve found leaking same to be check/overhaul/renew","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Discharge valve replaved with new spare valve received at Singapore.","2019-11-30","DRED190149","Completed","2019-11-23","No","No","No","Internal","Valve will be supplied in Singapore."]
[null,null,null,null,2465,"54_14/10/2019 11:42:04 PM","2019-08-05","Defect","Ship Staff","Ship Staff Insp.","Gas sampling system giving analysing pump failure alarm intermittently","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","Found Flowmeter ball valve stuck and blocking the flow, flowmeter opened and made the ball easy","2019-08-25","","Completed","2019-08-19","No","No","No","Internal"]
[null,null,null,null,2515,"54_16/10/2019 6:20:16 AM","2019-08-06","Defect","Ship Staff","Ship Staff Insp.","HP & LP Feed water retention dump valve found pin hole on the valve body","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","To repair/ renew the dump valve. Leak repaired.","2019-08-12","","Completed","2019-08-10","No","No","No","Internal"]
[null,null,null,null,2366,"54_2019-10-12 17:15:16.000","2019-08-07","Defect","Ship Staff","Ship Staff Insp.","Ship's Laundry thumble dryer on sunken deck and A-deck  found idler pulley damage and belt broken. Same to be renew/repair.","Elect. Mach. & Equip.","MLC Related","Equipment Related","","","","","Pulley and belt renewed.","2019-11-30","DRED190177","Completed","2019-11-27","No","No","No","Internal",""]
[null,null,null,null,583,"54_Tue Dec 10 2019 17:15:16 GMT+0000","2019-08-07","Breakdown","Ship Staff","Ship Staff Insp.","Ship's Laundry thumble dryer on sunken deck and A-deck  found idler pulley damage and belt broken. Same to be renew/repair.","Elect. Mach. & Equip.","MLC Related","Equipment Related","11.16","Low","","","Both laundry Dryer Idler pulley and belts replaced and checked workind satisfactory","2019-08-25","DRED190177","Completed","2019-11-27","No","No","No","Internal"]
[null,null,null,null,6279,"54_Sat Oct 12 2019 17:15:16 GMT+0000 (Coordinated Universal Time)","2019-08-07","Defect","Ship Staff","Ship Staff Insp.","Ship's Laundry thumble dryer on sunken deck and A-deck  found idler pulley damage and belt broken. Same to be renew/repair.","Elect. Mach. & Equip.","MLC Related","Equipment Related","","","","","Sunken deck and A deck laundry dryer idler pulley and belts replaced and checked working satisfactory.","2019-11-30","DRED190177","Completed","2019-11-27","No","No","No","Internal"]
[null,null,null,null,2472,"54_14/10/2019 11:57:41 PM","2019-08-09","Defect","Ship Staff","Ship Staff Insp.","No. 2 Eductor suction pressure guage needs to be calibrated.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","No. 2 Eductor suction pressure guage fluctuating during operation","2019-08-25","","Completed","2019-09-11","No","No","No","Internal"]
[null,null,null,null,2517,"54_16/10/2019 6:26:50 AM","2019-08-09","Defect","Ship Staff","Ship Staff Insp.","Sewage holding tank low low level testing switch seized.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Tank emptied and level switch dismantled and make it operational.","2019-08-26","","Completed","2019-08-20","No","No","No","Internal"]
[null,null,null,null,2524,"54_16/10/2019 6:36:35 AM","2019-08-09","Defect","Ship Staff","Ship Staff Insp.","DECK SEAL PUMP FOR CARGO SYSTEM, SUCTION VALVE BEFORE FILTER NOT HOLDING.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","To replace valve in drydock, job added in refman and removed from DDRL as per supeintendent instructions.","2019-12-15","","Completed","2019-09-02","No","No","No","Internal"]
[null,null,null,null,2525,"54_16/10/2019 6:38:01 AM","2019-08-09","Defect","Ship Staff","Ship Staff Insp.","OWS pump S.W priming valve not holding","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","To replace valve in drydock, job added in refman and removed from DDRL as per supeintendent instructions.","2019-09-02","","Completed","2019-09-02","No","No","No","Internal"]
[null,null,null,null,2530,"54_16/10/2019 6:43:57 AM","2019-08-10","Defect","Ship Staff","Ship Staff Insp.","Sewage holding Tank local level guage showing zero even when the tank is having content","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Level gauge checked and found float stucked up on the bottom and some hole on the upper side, same repaired with devcon.","2019-09-04","","Completed","2019-09-29","No","No","No","Internal"]
[null,null,null,null,2460,"54_14/10/2019 11:32:01 PM","2019-08-13","Defect","Ship Staff","Ship Staff Insp.","Breast Stbd winch oil pipe inlet and return line found leaking","Deck - Pipe / Fittings","General Appearance","Equipment Related","","","","","Leaking pipe dismantled and brought to engine workshop and the same renwed with new pipe of SCH80 and return line with SCH40.","2019-08-15","","Completed","2019-08-14","No","No","No","Internal"]
[null,null,null,null,2461,"54_14/10/2019 11:34:18 PM","2019-08-13","Defect","Ship Staff","Ship Staff Insp.","Soft patch on I.G. line","Inert Gas","Cargo / Ballast Systems","Equipment Related","","","","","Same to be attended when vessel is in gas free condition. It has been added in the dry-dock work list.","2019-08-15","","Completed","2019-08-15","No","No","No","Internal"]
[null,null,null,null,2462,"54_14/10/2019 11:36:10 PM","2019-08-13","Defect","Ship Staff","Ship Staff Insp.","Crack on the pipeline support forward of manifold","Deck - Pipe / Fittings","General Appearance","Equipment Related","","","","","Same to be attended when vessel is in gas free condition. It has been added in the dry-dock work list.\t","2019-08-15","","Completed","2019-08-15","No","No","No","Internal"]
[null,null,null,null,2467,"54_14/10/2019 11:46:21 PM","2019-08-13","Defect","Ship Staff","Ship Staff Insp.","Gear oil level less in port windlass gear box and port spring wich forward.","Deck - Mooring Machinery","Mooring","Equipment Related","","","","","Gear oil filled up.","2019-08-20","","Completed","2019-08-24","No","No","No","Internal"]
[null,null,null,null,2468,"54_14/10/2019 11:48:10 PM","2019-08-13","Defect","Ship Staff","Ship Staff Insp.","No. 2 Port side ECDIS giving SRB alarm","Navigation - ECDIS","Navigation","Equipment Related","","","","","Same is brought to the notice of the office and trouble shooting in underway.","2019-08-25","","Completed","2019-08-21","No","No","No","Internal"]
[null,null,null,null,2471,"54_14/10/2019 11:55:30 PM","2019-08-13","Defect","Ship Staff","Ship Staff Insp.","Cargo hose crane stbd side manual overriding limit for slewing protection of light post not working. Also hoisting winch  SWL 1t limit switch driving shaft pin broken.","Deck - Machinery","General Appearance","Equipment Related","","","","","Manual overriding valve rectified. Driving shaft pin and ball bearing renewed with new one. Tried out working satisfactory","2019-09-04","","Completed","2019-09-14","No","No","No","Internal"]
[null,null,null,null,2516,"54_16/10/2019 6:25:41 AM","2019-08-15","Defect","Ship Staff","Ship Staff Insp.","No2 FWG flowmeter found faulty","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Flow meter replaced with new spare.","2019-08-18","","Completed","2019-08-18","No","No","No","Internal"]
[null,null,null,null,2316,"54_17-10-2019 11:13:27","2019-08-21","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Drop Leakage near jacket water heater valves, to be cleaned and renewed if required","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","LT system water was drained in yard and at the time valve was opened up and the seal/o-ring renewed. LT system filled up and tested with pumps running, no more leakage.","2020-02-28","DRED190213","Completed","2020-02-27","Yes","No","No","Internal","Leakage is slight  and job will be carried out during EGCS installation docking."]
[null,null,null,null,2464,"54_14/10/2019 11:40:11 PM","2019-08-21","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Fuel injector testing area poster","LSA / FFA","Safety / LSA / FFA","Inappropriate Procedure","","","","","Superintendent internal audit observation. Poster pasted now near testing stand","2019-08-26","","Completed","2019-08-25","No","No","No","Internal"]
[null,null,null,null,2518,"54_16/10/2019 6:28:11 AM","2019-08-21","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Port boiler gauge glass light is not working","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Superintendent internal audit observation. Lamp replaced and defect closed","2019-08-26","","Completed","2019-08-24","No","No","No","Internal"]
[null,null,null,null,2519,"54_16/10/2019 6:30:19 AM","2019-08-21","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Emergency D/G radiator gauge glass opaque and level not visible","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","Superintendent internal audit observation. Water drained and guage glass cleaned","2019-08-31","","Completed","2019-08-26","No","No","No","Internal"]
[null,null,null,null,2520,"54_16/10/2019 6:31:31 AM","2019-08-21","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Both Aux boilers easing gear wire to be greased","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","Superintendent internal audit observation. Already greased and now completed","2019-09-05","","Completed","2019-08-26","No","No","No","Internal"]
[null,null,null,null,2521,"54_16/10/2019 6:32:44 AM","2019-08-21","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","no 2 A/C compressor belt slack and need retightening","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Superintendent internal audit observation. A/C compressor belt adjusted and job completed","2019-08-24","","Completed","2019-08-24","No","No","No","Internal"]
[null,null,null,null,2522,"54_16/10/2019 6:33:58 AM","2019-08-21","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","STP chlorination pump was running and no chemical passing through the tube","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Superintendent internal audit observation. Pump purged and rectified","2019-08-24","","Completed","2019-08-24","No","No","No","Internal"]
[null,null,null,null,2527,"54_16/10/2019 6:40:35 AM","2019-08-21","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ESB 440Volt insulation meter showing more than infinity","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","Superintendent internal audit observation. Checked and adjusted .","2019-09-21","","Completed","2019-09-06","No","No","No","Internal"]
[null,null,null,null,2528,"54_16/10/2019 6:41:46 AM","2019-08-21","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Stbd L.O bunker manifold valve wheel badly rusted and same to be renewed","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Superintendent internal audit observation. Rectified valve wheel chipped, buffed and painted.","2019-09-05","","Completed","2019-09-04","No","No","No","Internal"]
[null,null,null,null,2535,"54_17-10-2019 11:24:01","2019-08-21","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Observed abnormal noise with Economizer feed water pump no 1","E/R - Aux. Mach.,E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","Rubber bushes of coupling bolts renewed.","2019-10-31","DRED190213","Completed","2019-10-16","No","No","No","Internal"]
[null,null,null,null,2469,"54_14/10/2019 11:50:23 PM","2019-08-24","Defect","Ship Staff","Ship Staff Insp.","Forward electric whistle not working","Deck - Machinery","General Appearance","Equipment Related","","","","","Electric whistle opened and found bearing was damaged and ball came in contact between casing and connecting rod jamming the mechanical movement. The same was opened up and bearings renewed and made operational. While overhauling observed the shaft was in bad condition and spares have to be requested for future troubles","2019-09-24","","Completed","2019-08-27","No","No","No","Internal"]
[null,null,null,null,2317,"54_17/10/2019 10:21:56 AM","2019-08-25","Defect","Ship Staff","Ship Staff Insp.","One of the UTI tape ( out of 4)  is damaged The locking arrangement for operating lever is broken, Securing clips for cover are missing,Battery holder assey is missing","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.12","Medium","","","UTI Received at Singapore 02 June2020.","2020-02-28","DRED195067","Completed","2020-06-02","No","No","No","Internal","UTI tape is ready, will be connected at next opportunity."]
[null,null,null,null,2313,"54_2019-10-10 13:51:26.000","2019-09-07","Defect","Ship Staff","Ship Staff Insp.","Faulty X-Guard unit of Vapor monitoring system","Inert Gas","Cargo / Ballast Systems","Equipment Related","","","","","New X-guard unit fitted.","2019-11-30","DRED190211","Completed","2019-11-28","No","No","No","Internal",""]
[null,null,null,null,2319,"54_17/10/2019 10:30:23 AM","2019-09-07","Defect","Ship Staff","Ship Staff Insp.","Galley Hot Plate thermostat Faulty","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","11.13","Low","","","Replaced new thermostat and checked working satisfactory","2019-12-31","","Completed","2020-01-07","No","No","No","Internal","Has it not been received yet? Target date being revised till spare received?"]
[null,null,null,null,2531,"54_16/10/2019 6:45:15 AM","2019-09-11","Defect","Ship Staff","Ship Staff Insp.","ME indicator cocks 6 nos found chocked to be cleared/renew in port.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Indicator cocks dismantled and 2 nos replaced with new spare.","2019-09-24","","Completed","2019-09-22","No","No","No","Internal"]
[null,null,null,null,2532,"54_16/10/2019 6:46:25 AM","2019-09-11","Defect","Ship Staff","Ship Staff Insp.","WHRS port side HP inspection door packing observed sign of leakage, to be rectify.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","Inspection door packing renewed with new one.","2019-09-24","","Completed","2019-09-22","No","No","No","Internal"]
[null,null,null,null,2321,"54_17/10/2019 10:35:00 AM","2019-09-12","Defect","Ship Staff","Ship Staff Insp.","CCTV MONITOR NOT WORKING","Miscellaneous","Navigation","Equipment Related","7.12","High","","","CCTV monitor replaced on 25 Nov 2019. Working satisfactory","2019-11-30","DRED190191","Completed","2019-11-25","No","No","No","Internal","Will be supplied in Singapore."]
[null,null,null,null,2529,"54_16/10/2019 6:42:58 AM","2019-09-15","Defect","Ship Staff","Ship Staff Insp.","WHRS inspection door packing found gas leaking, packing/gasket to be check/replace.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Inspection door door packing replaced with new one.","2019-09-25","","Completed","2019-09-22","No","No","No","Internal"]
[null,null,null,null,6282,"54_31/10/2019 7:30:20 AM","2019-10-15","Defect","Ship Staff","Ship Staff Insp.","Provision crane manual overriding and limit switch found not operationl.","Deck - Machinery","Structural Condn. / WT integrity ","External Factors","8.5","Very High","","","Overhauled manual overriding lever and limit switch and made operational","2019-10-28","","Completed","2019-10-17","No","No","No","Internal"]
[null,null,null,null,2320,"54_17/10/2019 10:32:34 AM","2019-10-23","Defect","Ship Staff","Ship Staff Insp.","MSBD 5ET timer and ESBD timer faulty","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.37","Medium","","","Timer replaced with new spare","2020-01-30","","Completed","2020-01-21","No","No","No","Internal",""]
[null,null,null,null,6280,"54_Fri Nov 01 2019 11:40:06 GMT+0000 (Coordinated Universal Time)","2019-10-29","Critical Equipment","Owner / Marine / Tech. Suptd.","Ship Staff Insp.","Operational spares listed in HSQEEn 14.08.00.00.01 is just a minimum and vessel can assign additional spares as operational spares. For ex, ACB for MSB and ESB has been provided. These should also be marked as operational","Critical Equip.","Eng. / Strg. Comp.","Equipment Related","10.13","Very High","","","Issue will be reported in Master review as directed by office","2019-11-15","","Completed","2019-11-30","No","No","No","Internal","Comments related to QDMS should be menioned under master review. Please remove the defect from here and shift in Master's review."]
[null,null,null,null,2318,"54_17/10/2019 10:27:15 AM","2019-11-05","Defect","Ship Staff","Ship Staff Insp.","Garbage compactor PLC found not operational","Deck - Machinery","MARPOL Related","Equipment Related","10.37","Medium","","","Troubleshooted and found PLC not faulty.now made operational.","2020-02-28","DRED190246 (Received)","Completed","2020-06-15","No","No","No","Internal",""]
[null,null,null,null,7488,"54_Tue Nov 12 2019 07:02:03 GMT+0000 (Coordinated Universal Time)","2019-11-09","Defect","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","Vessel was fitted with 1.5 tons SWL davit on forecastle and 2.5 tons SWL davit for pumproom. There was no evidence of load test with in 5 years.","Deck - Machinery","Cert. & Docu.","Equipment Related","8.5","Very High","","","Ship's staff have carried out the load test on board with LOADCELL to 1.25 times SWL of both the davits and record maintained.","2019-12-09","","Completed","2019-11-30","No","No","No","External"]
[null,null,null,null,7489,"54_Wed Dec 11 2019 06:52:30 GMT+0000 (Coordinated Universal Time)","2019-11-09","Defect","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","Vessel was provided with 3 tankscopes. However there was no evidence that these were being calibrated  for volume","Miscellaneous","Cargo / Ballast Systems","Equipment Related","5.23","Very High","","","The calibration was carried out on monthly basis as per manufacterer's instructions. the details of span gases used for calibration are also being included in the monthly calibration sheet","2019-12-09","","Completed","2019-11-10","No","No","No","External"]
[null,null,null,null,7490,"54_Tue Nov 12 2019 07:10:06 GMT+0000 (Coordinated Universal Time)","2019-11-09","Defect","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","Stbd. anchor brake tightening system was hydraulic. Spring tightening indicators on spindle and plate were not aligned and had a gap of about 10-12cm.","Deck - Mooring Machinery","Mooring","Equipment Related","9.2","Very High","","","After departure stbd anchor was lashed/secured in position and as per guidance given in the makers manual the spring tension indicator(pointer)on the spindle  was bought in line with the indicator plate. ","2019-12-09","","Completed","2019-11-13","No","No","No","External"]
[null,null,null,null,7491,"54_Thu Dec 12 2019 03:48:04 GMT+0000 (Coordinated Universal Time)","2019-11-09","Defect","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","Vessel was fitted with ballast water treatment plant.However there was no evidence that is was being used.\t\t\t","Documentation","Cargo / Ballast Systems","Equipment Related","6.21","High","","","The system is not being used as vessel is complying with the D1 regulation of the Ballast water convention.","2019-12-09","","Completed","2019-11-30","No","No","No","External"]
[null,null,null,null,6283,"54_15/11/2019 09:02:18 AM","2019-11-09","Defect","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","STBD anchor break tightening system, spring tightening indicator on spindle & plate were not aligned ","Deck - Machinery","Mooring","Equipment Related","9.2","Very High","","","Alignment of windlass hydraulic break carried out, Spring tension marking on spindle aligned with the set marking.","2019-11-15","","Completed","2019-11-10","No","No","No","External"]
[null,null,null,null,7444,"54_15/12/2019 02:26:07 PM","2019-11-15","Defect","Ship Staff","Ship Staff Insp.","During wet rounds it was observed that the hoisting wire for E/R skylight was damaged & requires replacement.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","Damaged wire replaced with spare wire of similar specification.","2019-12-30","","Completed","2019-12-23","No","No","No","Internal"]
[null,null,null,null,7450,"54_43748.5773842593","2019-11-18","Defect","Ship Staff","Ship Staff Insp.","Hydraulic Leak observed in aft spring line mooring winch - return pipeline ","Deck - Mooring Machinery","Mooring","Equipment Related","9.14","Medium","","","Leaking hydraulic pipe renewed on 03 Dec 2019","2020-01-31","","Completed","2019-12-03","No","No","No","Internal"]
[null,null,null,null,7447,"54_Sat Jan 12 2019 10:35:47 GMT+0000 (Coordinated Universal Time)","2019-11-22","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Stbd side gangway angle indicator found frozen.","Miscellaneous","General Appearance","Equipment Related","","","","","P & S Gangway angle indicator overhauled","2020-02-22","","Completed","2019-11-30","No","No","No","Internal"]
[null,null,null,null,7448,"54_Sat Jan 12 2019 10:39:12 GMT+0000 (Coordinated Universal Time)","2019-11-22","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","TMC operating procedure was not displayed in wheel house.","Navigation - Others","Navigation","Human Error","4.9","Medium","","","TMC Operating procedure laminated & posted","2020-02-22","","Completed","2019-11-29","No","No","No","Internal"]
[null,null,null,null,7449,"54_43748.5210185185","2019-11-22","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","A deck Crew laundry: Electric power supply switch found broken.","Elect. Mach. & Equip.","General Appearance","Equipment Related","10.37","Medium","","","Defected switch replaced with new spare ","2020-02-22","","Completed","2019-11-25","No","No","No","Internal"]
[null,null,null,null,7451,"54_Tue Mar 12 2019 23:03:53 GMT+0000 (Coordinated Universal Time)","2019-11-22","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Various winch platform grating on deck need to derust and paint.","Deck - Pipe / Fittings","General Appearance","Inappropriate Procedure","","","","","Derusting & painting carried out of M2, M3 winch platform after departure Singapore","2020-01-07","","Completed","2019-12-01","No","No","No","Internal"]
[null,null,null,null,6277,"54_Thu Oct 10 2019 12:30:16 GMT+0000 (Coordinated Universal Time)","2019-11-22","Defect","Ship Staff","Suptd. Insp.","No.2 Cargo eductor pressure reading erratic in CCR display during operation","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.13","Medium","","","Pressure guage /transimitter blow checked, inlet connection removed and cleared.Transimiter air blowoff carried out.Pressure reading showing normal value.","2020-02-22","","Completed","2019-12-18","No","No","No","Internal"]
[null,null,null,null,7436,"54_Fri Apr 12 2019 19:31:30 GMT+0000 (Coordinated Universal Time)","2019-11-23","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Aux boiler fuel supply pump seal leaking","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Pump stopped and inspected, minor leak at shaft and job planned After departure port","2019-12-31","","Completed","2019-12-17","No","No","No","Internal","Why fuel pump job needs to wait after discharge . Must be attended prior that if vessel has mechanical seal."]
[null,null,null,null,7437,"54_Fri Apr 12 2019 19:40:27 GMT+0000 (Coordinated Universal Time)","2019-11-23","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Removed ME fuel valves are not overhauled.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","All spare fuel valves overhauled and pressure tested.","2019-12-31","","Completed","2019-12-19","No","No","No","Internal","How many valves already overhauled and how many remaining must be mentioned in \"action taken\""]
[null,null,null,null,7438,"54_Fri Apr 12 2019 20:05:59 GMT+0000 (Coordinated Universal Time)","2019-11-23","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Used DG Liner to land for honing","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Landed during Singapore  transit on 06 Jan2020 for reconditioning","2020-01-08","","Completed","2020-01-06","No","No","No","Internal"]
[null,null,null,null,7439,"54_Wed Dec 04 2019 20:54:30 GMT+0000 (Coordinated Universal Time)","2019-11-23","Defect","Owner / Marine / Tech. Suptd.","Ship Staff Insp.","Water leaking drop wise from the aft ME air cooler. leak was from one of the stud of the end plate of feed water heater.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","At YiuLian shipyard, the Aft pre-heaterfwd end cover removed. Broken stud extracted and fitted with new stud. Cover and sealing faces cleaned and boxed back with new gasket. Water tried out and no more leakage.","2020-02-23","","Completed","2020-02-22","No","No","No","Internal"]
[null,null,null,null,7440,"54_Sun May 12 2019 07:39:55 GMT+0000 (Coordinated Universal Time)","2019-11-23","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ME Exhaust uptake pipe insulation is deteriorated at varoius place near leaking bellow, metal sheet to rivet in place of damaged insulation","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Two part  metal sheet riveted to cover the damaged uptake pipe insulation near bellow.","2019-12-31","","Completed","2019-12-18","No","No","No","Internal","Well noted. Target date revised as job required staging and same is planned."]
[null,null,null,null,7441,"54_Sun May 12 2019 06:46:25 GMT+0000 (Coordinated Universal Time)","2019-11-23","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Echo sounder cannot print in auto mode at regular intervals.","Navigation - Echo Sounder / Speed Log","Navigation","Equipment Related","4.7","High","","","AS per service technician echo sounder is in good order and if the auto print function is required need to change the ROM chip to the latest version.","2020-02-22","","Completed","2020-06-02","No","No","No","Internal","We will get it attended this call Singapore."]
[null,null,null,null,7442,"54_Thu Dec 05 2019 07:46:17 GMT+0000 (Coordinated Universal Time)","2019-11-23","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Port anchor chain found twisted.","Deck - Mooring Machinery","Mooring","Equipment Related","9.2","Very High","","","P-Anchor cable twist rectified at Quanzhou, Anchorage.","2020-02-22","","Completed","2019-12-26","No","No","No","Internal"]
[null,null,null,null,7452,"54_Tue Mar 12 2019 23:07:05 GMT+0000 (Coordinated Universal Time)","2019-11-23","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Flash light at pump room bottom platform found damaged & to be replaced","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","Defective flash light replaced with new flash light at pump room bottom","2019-11-28","","Completed","2019-11-25","No","No","No","Internal"]
[null,null,null,null,7453,"54_Fri Apr 12 2019 19:35:41 GMT+0000 (Coordinated Universal Time)","2019-11-23","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Control air drier auto drain filter pipe missing","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","New pipe fitted","2019-11-29","","Completed","2019-11-26","No","No","No","Internal"]
[null,null,null,null,7454,"54_Fri Apr 12 2019 19:48:37 GMT+0000 (Coordinated Universal Time)","2019-11-23","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Insulating mat near IG valve near EGB is oil soaked. Oil leak to identify and rectify. Insulating mat to renew or clean.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","Insulating mat changed and oil leak rectified.","2019-11-28","","Completed","2019-11-27","No","No","No","Internal"]
[null,null,null,null,7455,"54_Fri Apr 12 2019 19:52:13 GMT+0000 (Coordinated Universal Time)","2019-11-23","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Insulation mat near EGB soot blower is deteriorated. To be renewed.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","Mat changed","2019-11-28","","Completed","2019-11-27","No","No","No","Internal"]
[null,null,null,null,7456,"54_Fri Apr 12 2019 19:58:16 GMT+0000 (Coordinated Universal Time)","2019-11-23","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","A vent cock is fitted in incinerator settling tank steam inlet line. Live steam leaking from the cock.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","Steam leak rectified.","2019-12-08","","Completed","2019-11-26","No","No","No","Internal"]
[null,null,null,null,7457,"54_Fri Apr 12 2019 20:01:32 GMT+0000 (Coordinated Universal Time)","2019-11-23","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","T G sump vent to paint","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","T G sump vent painted","2019-12-08","","Completed","2019-11-27","No","No","No","Internal"]
[null,null,null,null,7458,"54_Fri Apr 12 2019 20:11:19 GMT+0000 (Coordinated Universal Time)","2019-11-23","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Workshop door stencil has faded. To re-stencil","Miscellaneous","Eng. / Strg. Comp.","Inappropriate Procedure","","","","","Re-stenciled","2019-12-03","","Completed","2019-11-27","No","No","No","Internal"]
[null,null,null,null,7459,"54_Fri Apr 12 2019 20:14:00 GMT+0000 (Coordinated Universal Time)","2019-11-23","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Citadel toilet to clean","Miscellaneous","Eng. / Strg. Comp.","Human Error","","","","","Citadel toilet cleaned.","2019-12-08","","Completed","2019-11-29","No","No","No","Internal"]
[null,null,null,null,7460,"54_Fri Apr 12 2019 20:20:37 GMT+0000 (Coordinated Universal Time)","2019-11-23","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","OWS Flocculaqtion tank is left with all foam floating. Clean always after completion of operation, floating foam to be removed. Engineers to train. Leaking area of the flocculation tank to repair.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","OWS flocculation tank cleaned. Engineers trained. Flocculation tank leak rectified.","2019-12-08","","Completed","2019-11-27","No","No","No","Internal"]
[null,null,null,null,7461,"54_Fri Apr 12 2019 20:25:16 GMT+0000 (Coordinated Universal Time)","2019-11-23","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Stbd side structure of DG area needs to claen","Miscellaneous","Eng. / Strg. Comp.","Human Error","","","","","Stbd side structure of DG area cleaned.","2019-11-23","","Completed","2019-11-29","No","No","No","Internal"]
[null,null,null,null,7462,"54_Fri Apr 12 2019 20:28:56 GMT+0000 (Coordinated Universal Time)","2019-11-23","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Elevator room to clean","E/R - Aux. Mach.","Eng. / Strg. Comp.","Human Error","","","","","Elevator room cleaned","2019-12-03","","Completed","2019-11-28","No","No","No","Internal"]
[null,null,null,null,7463,"54_Fri Apr 12 2019 20:34:59 GMT+0000 (Coordinated Universal Time)","2019-11-23","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Flash light at pump room bottom platform to renew.","Miscellaneous","Cargo / Ballast Systems","Equipment Related","","","","","Flash light at pump room bottom platform renewed.","2019-11-28","","Completed","2019-11-25","No","No","No","Internal"]
[null,null,null,null,7464,"54_Fri Apr 12 2019 20:41:29 GMT+0000 (Coordinated Universal Time)","2019-11-23","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Accomodation gas detection system is in alarm condition with path block alarm. To rectify","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","Accomodation gas detection system alarm rectified.","2019-12-03","","Completed","2019-11-26","No","No","No","Internal"]
[null,null,null,null,7465,"54_Fri Apr 12 2019 20:46:26 GMT+0000 (Coordinated Universal Time)","2019-11-23","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","VECS panel on deck inside and exterior to clean. Pressure gauge to renew.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","VECS panel on deck inside and exterior to cleaned and pressure gauge renewed.","2019-12-08","","Completed","2019-11-29","No","No","No","Internal"]
[null,null,null,null,7466,"54_Fri Apr 12 2019 21:05:09 GMT+0000 (Coordinated Universal Time)","2019-11-23","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Water found collected aft of LO cooler. Water source to identify and rectify.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","Water source to indenfied and rectified.","2019-12-03","","Completed","2019-11-29","No","No","No","Internal"]
[null,null,null,null,7467,"54_Sun May 12 2019 07:29:58 GMT+0000 (Coordinated Universal Time)","2019-11-23","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Hydraulic line of winch , which is leaking to be renewed.","Deck - Pipe / Fittings","Mooring","Equipment Related","11.4","Very High","","","Pipeline was renewed and replaced","2019-12-03","","Completed","2019-12-03","No","No","No","Internal"]
[null,null,null,null,7468,"54_Sun May 12 2019 07:55:53 GMT+0000 (Coordinated Universal Time)","2019-11-23","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Port side cargo manifold no.1, reducer 26” x 10”- found rusty. ","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.49","High","","","Derusting and painting of reducer carried out and completed.","2019-12-03","","Completed","2019-12-01","No","No","No","Internal"]
[null,null,null,null,7469,"54_Thu Dec 05 2019 08:42:06 GMT+0000 (Coordinated Universal Time)","2019-11-23","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Various exhaust uptakes silver paint has peeled off, to paint same.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Peeled off paint scraped from uptakes,cleaned & painted","2019-12-24","","Completed","2019-12-05","No","No","No","Internal"]
[null,null,null,null,7493,"54_Tue Mar 12 2019 23:09:49 GMT+0000 (Coordinated Universal Time)","2019-11-23","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Pump room entrance locker to paint. Side shells of port side to clean off dust.","Miscellaneous","General Appearance","Inappropriate Procedure","","","","","Completed painting cabinet at pumproom entrance & cleaning pump room stringers from top to bottom","2019-12-03","","Completed","2019-12-13","No","No","No","Internal"]
[null,null,null,null,7494,"54_Tue Mar 12 2019 23:11:42 GMT+0000 (Coordinated Universal Time)","2019-11-23","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Mooring wires are covered with mud, to clean.","Deck - Mooring Machinery","General Appearance","Inappropriate Procedure","","","","","All mooring wires washed & prepared for greasing ","2020-01-22","","Completed","2019-12-14","No","No","No","Internal"]
[null,null,null,null,7495,"54_Thu Dec 05 2019 08:30:10 GMT+0000 (Coordinated Universal Time)","2019-11-23","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Top of Soot collecting tank to clean and paint","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","CLeaned and painted","2019-12-14","","Completed","2019-12-14","No","No","No","Internal"]
[null,null,null,null,7485,"54_Tue Nov 12 2019 06:11:05 GMT+0000 (Coordinated Universal Time)","2019-11-25","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","12.20.05.011.04 - Pre Arrival and Commencement of Cargo checklist for 24 Sept 2019 signed by C/O and Master, however time of completion of checklist Sec D missing. ","Documentation","Cert. & Docu.","Inappropriate Procedure","","","","","Missing enty for completion timing fo checklist 12.20.05.011.04 Section D filled in checklist","2020-02-24","","Completed","2019-11-29","No","No","No","Internal"]
[null,null,null,null,7486,"54_Tue Nov 12 2019 06:39:52 GMT+0000 (Coordinated Universal Time)","2019-11-25","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Checklist 12.80.13.094.00 mentioned completed on 24 Sep 2019 in CCR Movement book is meant for Chemical Tankers. (12.80.xx.xx.xx Chemical Tanker Guidelines)","Miscellaneous","Cert. & Docu.","Inappropriate Procedure","","","","","For completion of cargo operation, 2 checklist were being filed & entries made in the CCR log. Checklist (12.80.13.094.00 & 12.20.05.341.00).  Henceforth12.80.13.094.00 will be discontinued. ","2020-02-24","","Completed","2019-11-29","No","No","No","Internal"]
[null,null,null,null,7487,"54_Tue Nov 12 2019 06:43:47 GMT+0000 (Coordinated Universal Time)","2019-11-25","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","- Pre arrival and commencement of cargo operation checklist for loading at Jubilee Sec B (24 Hrs Prior Operation) completed on 21 Sep at 1500 Hrs, however Operations commenced on 24 Sep 2019.\n\nSection B to be reviewed and re-signed in case cargo operations is delayed after arrival.\n\n","Miscellaneous","Cert. & Docu.","Inappropriate Procedure","","","","","Remark made in checklist 12.20.05.011.04 section B. Reviewed on 22- Sep-2019/ 1600LT. And entries made in CCR Log for the same.","2020-02-24","","Completed","2019-11-29","No","No","No","Internal"]
[null,null,null,null,7496,"54_15/12/2019 1:55:04 PM","2019-12-02","Defect","Ship Staff","Ship Staff Insp.","Main DG No.1 Air cooler tubes leaking","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Air cooler removed and tubes checked, leaky tubes plugged","2019-12-03","","Completed","2019-12-03","No","No","No","Internal"]
[null,null,null,null,7497,"54_15/12/2019 1:59:06 PM","2019-12-08","Defect","Ship Staff","Ship Staff Insp.","Emergency generator exaust pipe spark arrestor mesh found damaged","Deck - Pipe / Fittings","Emgcy. Systems","Equipment Related","","","","","Mesh renewed","2019-12-09","","Completed","2019-12-09","No","No","No","Internal"]
[null,null,null,null,7443,"54_15/12/2019 02:18:52 PM","2019-12-12","Defect","Ship Staff","Ship Staff Insp.","Minor leak observed in hydraulic line for valve operation return line.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","6.4","High","","","Leaking pipe replaced with new pipe fabricated onboard","2019-12-31","","Completed","2019-12-18","No","No","No","Internal","Please renew the pipe on priority basis well before discharge port."]
[null,null,null,null,7492,"54_15/12/2019 02:23:28 PM","2019-12-15","Defect","Ship Staff","Ship Staff Insp.","During monthly calibratio of portable gas meters it was noted that 1 sensor for honeywell gas meter was faulty & required replacement","Miscellaneous","Safety / LSA / FFA","Equipment Related","5.23","Very High","","","Faulty sensor replaced with spare sensor avalable onboard. Equipment tested & calibrated after sensor replacement, found in good working condition","2019-12-18","","Completed","2019-12-15","No","No","No","Internal"]
[null,null,null,null,9479,"54_09/01/2020 06:28:16 PM","2019-12-30","Defect","Ship Staff","Ship Staff Insp.","4S AFT COW machine found not operational during discharging operation at Quanzhou, China","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.34","High","","","COW machine overhauled, driving unit gear found wornout, same replaced with spare driving gear & COW machine tested manually, found in good working condition","2020-04-30","","Completed","2020-01-08","No","No","No","Internal"]
[null,null,null,null,9477,"54_09/01/2020 06:48:30 PM","2020-01-07","Breakdown","Ship Staff","Ship Staff Insp.","Manual sounding/dipping rod tape found damaged/cracked at 2 locations along the length of the tape.","Miscellaneous","Cargo / Ballast Systems","Equipment Related","8.13","Medium","","","Defected tape replaced with new spare tape.","2020-01-31","","Completed","2020-01-07","No","No","No","Internal"]
[null,null,null,null,9478,"54_09/01/2020 06:39:59 PM","2020-01-07","Defect","Ship Staff","Ship Staff Insp.","P & S Bridge wing doors found very Hard to operate. Roller bearings requires replacement.","Accommodation","General Appearance","Equipment Related","11.6","Medium","","","Roller bearings for P & S bridge wing doors replaced with new bearings.","2020-01-30","","Completed","2020-01-09","No","No","No","Internal"]
[null,null,null,null,10176,"54_26/01/2020 10:39:33 AM","2020-01-26","Breakdown","Ship Staff","Ship Staff Insp.","Main air compressor No.1 Breakdown","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","New spares were received at S'pore transit and compressor was boxed back using new spares. Makers instructions were followed in assembly of the compressor. Compressor tried out and all found satisfactory. Will be kept under close observation.","2020-02-28","DRED200004 , DRED 200027","Completed","2020-02-07","No","No","No","Internal"]
[null,null,null,null,11479,"54_22-04-2020 20:11:09","2020-02-01","Defect","Ship Staff","Ship Staff Insp.","Water fountain in engine room and officers mess not operative.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","New water fountain received at yulian and  installed.","2020-04-01","DRED200042","Completed","2020-03-29","No","No","No","Internal"]
[null,null,null,null,11480,"54_22-04-2020 20:21:59","2020-02-05","Defect","Ship Staff","Ship Staff Insp.","Washing machine in officers laundry at C deck had abnormal noise, Bearings to be renewed for drum.","Accommodation","MLC Related","Equipment Related","11.16","Low","","","Bearings received in Yulian DD and same replaced and now operational.","2020-04-15","DRED200072","Completed","2020-03-31","No","No","No","Internal"]
[null,null,null,null,16191,"54_18/12/2020 09:24:12 AM","2020-02-10","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Steam heating pipes deck penetration to derust and paint","Deck - Pipe / Fittings","General Appearance","Behaviour Based","11.4","Very High","","","Derusting and painting carried out on Steam heating pipes deck penetration .","2020-04-10","","Completed","2020-03-14","No","No","No","Internal"]
[null,null,null,null,16192,"54_18/12/2020 09:31:35 AM","2020-02-10","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Deck pipeline Supports to derust & paint","Deck - Pipe / Fittings","General Appearance","Inappropriate Procedure","11.5","Medium","","","Deck pipeline Supports  derusted & painted","2020-04-10","","Completed","2020-03-21","No","No","No","Internal"]
[null,null,null,null,16193,"54_18/12/2020 09:52:21 AM","2020-02-10","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Main deck hydraulic lines underside to derust & paint","Deck - Pipe / Fittings","General Appearance","Behaviour Based","11.5","Medium","","","Main deck hydraulic lines underside  derusted & painted","2020-04-10","","Completed","2020-03-21","No","No","No","Internal"]
[null,null,null,null,16194,"54_18/12/2020 01:53:15 PM","2020-02-10","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","PV valves\tPipe flanges to derust & paint","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.21","High","","","PV valves\tPipe flanges  derusted & painted","2020-04-10","","Completed","2020-03-31","No","No","No","Internal"]
[null,null,null,null,16195,"54_18/12/2020 01:57:10 PM","2020-02-10","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Pipe Support on deck to derust & paint","Deck - Pipe / Fittings","General Appearance","Behaviour Based","11.5","Medium","","","Pipe Support on deck  derusted & painted","2020-04-10","","Completed","2020-03-24","No","No","No","Internal"]
[null,null,null,null,16196,"54_18/12/2020 02:00:12 PM","2020-02-10","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","COT 3S COW Machine (FWD) pipeline support wasted & holed part to renew – ship staff can do it after departure from yard as COT will be gas free","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.5","Medium","","","COT 3S COW Machine (FWD) pipeline support fabricated and renewed.","2020-05-10","","Completed","2020-04-04","No","No","No","Internal"]
[null,null,null,null,16197,"54_18/12/2020 02:03:33 PM","2020-02-10","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Mooring Winches Foundation to derust & paint","Deck - Mooring Machinery","Mooring","Equipment Related","9.14","Medium","","","Mooring Winches Foundation derusted & painted","2020-04-10","","Completed","2020-04-07","No","No","No","Internal"]
[null,null,null,null,16198,"54_18/12/2020 02:18:51 PM","2020-02-10","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Dust Bin \tKept at cargo pump room entrance –to secure & mark for type of garbage to put in","Miscellaneous","General Appearance","Human Error","6.2","High","","","Dust bin at the cargo pumproom entrace secured and marked for the category of garbage.","2020-02-17","","Completed","2020-02-14","No","No","No","Internal"]
[null,null,null,null,16199,"54_18/12/2020 02:31:33 PM","2020-02-10","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","COP #3\tLower seal minor oil leakage, to investigate and rectify","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.8","Medium","","","COP No.3 TESTED AND TRIED OUT DURING PRE ARRIVAL TEST, No leaks found","2020-05-10","","Completed","2020-05-06","No","No","No","Internal"]
[null,null,null,null,16200,"54_18/12/2020 02:40:44 PM","2020-02-10","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","At poop deck gear LO sight class to clean","Deck - Mooring Machinery","Mooring","Equipment Related","9.17","High","","","LO sight class cleaned and refitted at the Poop deck","2020-03-10","","Completed","2020-03-20","No","No","No","Internal"]
[null,null,null,null,16201,"54_18/12/2020 4:44:38 PM","2020-02-10","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","FO pump ( aft seal leaking)","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.28","Low","","","Seal  to be renewed. Target date revised to 10th July. Item re- raised on 8th July.","2020-04-10","","Completed","2020-07-08","No","No","No","Internal"]
[null,null,null,null,16202,"54_18/12/2020 4:48:01 PM","2020-02-10","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Top bracing air regulator leakage.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Job in hand. Regulator renewed.","2020-04-10","","Completed","2020-03-15","No","No","No","Internal"]
[null,null,null,null,16203,"54_18/12/2020 4:56:13 PM","2020-02-10","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ME JCW pre heater thermometer illegible.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Job in hand. Thermometer renewed.","2020-03-10","","Completed","2020-02-27","No","No","No","Internal"]
[null,null,null,null,16204,"54_18/12/2020 5:00:20 PM","2020-02-10","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","16k Steam supply to COPT &WBPT valve gland leaking.","Deck - Pipe / Fittings","Eng. / Strg. Comp.","Equipment Related","10.28","Low","","","Job in hand. Gland repacked.","2020-04-10","","Completed","2020-03-15","No","No","No","Internal"]
[null,null,null,null,16205,"54_18/12/2020 5:07:47 PM","2020-02-10","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","TG CSW suction chest valve gland leaking","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.31","Very High","","","Gland packing to be renewed.Gland repacked.","2020-04-10","","Completed","2020-03-03","No","No","No","Internal"]
[null,null,null,null,16206,"54_18/12/2020 5:03:38 PM","2020-02-10","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","FO pump No.4 flange leaking.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.28","Low","","","To be done at suitable opportunity. Leak repaired.","2020-04-10","","Completed","2020-03-10","No","No","No","Internal"]
[null,null,null,null,11475,"54_22-04-2020 21:19:19","2020-03-01","Defect","Ship Staff","Ship Staff Insp.","BWTS gas detection system found to be defective giving Fault 3 analysing pump and internal leakage alarm.","Deck - Machinery,Deck - Pipe / Fittings","Eng. / Strg. Comp.","Equipment Related","6.22","Medium","","","All alarms torubleshooted and all operational.","2020-08-30","","Completed","2020-08-03","No","No","No","Internal","Since you have tried every thing . But till it trips in 12 hours. Send a mail with you action taken. I will seek advise from maker."]
[null,null,null,null,10175,"54_26/01/2020 10:24:55 AM","2020-03-25","Defect","Ship Staff","Ship Staff Insp.","Workshop Package Air con blower defective","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Blower removed -same is sealed unit with Motor Blower Unit, found seized,Require nw spare-requisition raised.SPARE RECEIVED JOB IN HAND. TARGET DATE REVISED TO 30TH SEPT. Blower renewed on 20-08-20","2020-09-30","DRED200006","Completed","2020-08-20","No","No","No","Internal","Readiness is in Aug 20"]
[null,null,null,null,11481,"54_22-04-2020 20:26:55","2020-04-01","Defect","Ship Staff","Ship Staff Insp.","Aux engine no 2 Exhaust piping flange to EGCS system found to be leaking.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.28","Low","","","Cladding, laggings removed found all the bolts were slack, same retightened and engine started to check for further leaks and found everything in order.","2020-04-07","","Completed","2020-04-02","No","No","No","Internal"]
[null,null,null,null,11476,"54_22-04-2020 20:33:32","2020-04-06","Defect","Ship Staff","Ship Staff Insp.","During monthly inspection of compressor found big end bearing of HP piston in the verge of breakdown.","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","compressor dismantled, float test done, both big end bearing of HP & LP renewed and under observation. found bearing dust in L.O after test run and in observation to check it doesnt not aggrevate. compressor oil replenished and now no more bearing dust appearing. will still carry out monthly inspection and if there is any abnormality will inform office and closing the job has completed now.","2020-05-15","","Completed","2020-05-05","No","No","No","Internal"]
[null,null,null,null,11482,"54_22-04-2020 20:37:48","2020-04-06","Defect","Ship Staff","Ship Staff Insp.","During ER rounds found minor leakage from Servo oil pump (Port side) high pressuredischarge line.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.28","Low","","","During port stay L.O pumps stopped and H.P pipe of Servo oil pump dismantled , Claw, thrust collar and sealing faces cleaned and o -rings renewed.","2020-04-20","","Completed","2020-04-15","No","No","No","Internal"]
[null,null,null,null,11483,"54_22-04-2020 20:41:49","2020-04-10","Defect","Ship Staff","Ship Staff Insp.","No 2 Booster pump motor had abnormal noise and bearings to be renewed.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","No 2 booster pump motor was overhauled at port stay and bearing renewed and now motor operates smooth.","2020-04-21","","Completed","2020-04-16","No","No","No","Internal"]
[null,null,null,null,11484,"54_22-04-2020 20:44:38","2020-04-11","Defect","Ship Staff","Ship Staff Insp.","ME LO autoback wash filter ratchet mechanism assembly shaft had oil seepage. X ring to be renewed.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.28","Low","","","X ring and o rings of shaft  ratchet mechanism renewed and now found in order","2020-04-20","","Completed","2020-04-17","No","No","No","Internal"]
[null,null,null,null,11485,"54_22-04-2020 20:51:31","2020-04-12","Defect","Ship Staff","Ship Staff Insp.","FWG feed line copper pipe leaking at connections","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.28","Low","","","FWG feed line connections renewed and leakages rectified.","2020-04-27","","Completed","2020-04-19","No","No","No","Internal"]
[null,null,null,null,11486,"54_22-04-2020 20:59:16","2020-04-12","Defect","Ship Staff","Ship Staff Insp.","Various steam leakages in engine room identified.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.28","Low","","","Steam leakages in engine room identified and rectified.","2020-04-25","","Completed","2020-04-18","No","No","No","Internal"]
[null,null,null,null,11477,"54_22-04-2020 21:15:01","2020-04-14","Defect","Ship Staff","Ship Staff Insp.","During routine fuel valve testing of no 2 AE observed the valve to be stuck in cylinder head","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Tried out taking out even with hydraulic jacks. Fuel valve found to be stuck badly, remvoing cylinder head to replace injector. Cylinder head removed and replaced with newly overhauled cylinder head.","2020-04-30","","Completed","2020-05-03","No","No","No","Internal"]
[null,null,null,null,11487,"54_22-04-2020 21:11:50","2020-04-15","Defect","Ship Staff","Ship Staff Insp.","Sealing air fan for WHRS had abnormal nosie.","E/R - Aux. Mach.,E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Sealing air fan blower dismantled physically cleaned and sealing air motor overhauled and now operating smooth.","2020-04-30","","Completed","2020-04-19","No","No","No","Internal"]
[null,null,null,null,11478,"54_22-04-2020 21:27:04","2020-04-22","Defect","Ship Staff","Ship Staff Insp.","OWS pipe before 3 way valve found to be leaking.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.31","Very High","","","Pipe removed jigged and new pipe welded to existing pipe and rectified.","2020-04-30","","Completed","2020-05-02","No","No","No","Internal"]
[null,null,null,null,11577,"54_01/05/2020 4:20:45 PM","2020-04-26","Defect","Ship Staff","Ship Staff Insp.","WHRS casing door gasket leaking. Leak to be rectified by renewing door packing.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.28","Low","","","WHRS door gasket renewed","2020-05-15","","Completed","2020-05-08","No","No","No","Internal"]
[null,null,null,null,11576,"54_01/05/2020 4:24:29 PM","2020-04-27","Defect","Ship Staff","Ship Staff Insp.","Boiler Blowdown valve gasket and glandpacking leaking","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.28","Low","","","Boiler blowdown valve glandpacking and gasket renewed. Later noticed the water was leaking from crack in the pipe. Pipe was removed and taken to workshop where it was welded and now leakage is rectified.","2020-05-30","","Completed","2020-05-05","No","No","No","Internal"]
[null,null,null,null,11578,"54_01/05/2020 4:27:53 PM","2020-04-30","Defect","Ship Staff","Ship Staff Insp.","Various steam leaks in engine room to be rectified. 1.) steam leak above TG vaccum condensor 2) Steam leak above LO transfer pump 3) Steam leak above TG dump valve","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.28","Low","","","All mentioned steam leaks has been rectified.","2020-06-30","","Completed","2020-05-24","No","No","No","Internal"]
[null,null,null,null,11835,"54_15-05-2020 16:56:53","2020-05-01","Defect","Ship Staff","Ship Staff Insp.","FWG inlet to distillate pump from condensor piping has crack same to be removed and welded in workshop.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","FWG pipe dismantled adn brought to workshop for welding, welding completed and same has been put in place. Tried out.","2020-05-22","","Completed","2020-05-17","No","No","No","Internal"]
[null,null,null,null,11832,"54_15-05-2020 17:10:35","2020-05-02","Critical Equipment,Defect","Ship Staff","Ship Staff Insp.","Emergency fire pump operational satisfactory but priming device is engaging sluggish during starting same needs to be investigated.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Emergency fire pump priming device spring casing removed and dismantled.Found spring broken and O-ring damaged. Same replaced using new spares from kit. Tried out.Found satisfactory.","2020-06-09","","Completed","2020-05-18","No","No","No","Internal"]
[null,null,null,null,11833,"54_15-05-2020 17:04:52","2020-05-04","Defect","Ship Staff","Ship Staff Insp.","Ows flotation tank leaking and same needs replacement.","Critical Equip.,E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","6.17","Very High","","","Tank received and renewed.","2021-05-28","DRED200081","Completed","2021-05-01","No","No","No","Internal"]
[null,null,null,null,11836,"54_15-05-2020 16:48:00","2020-05-05","Defect","Ship Staff","Ship Staff Insp.","No 1 COPT L.O cooler oil was leaking from cooler flange.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.28","Low","","","Cooler flange tightened and oil leakage arrested.","2020-06-15","","Completed","2020-05-12","No","No","No","Internal"]
[null,null,null,null,11837,"54_15-05-2020 16:44:00","2020-05-08","Critical Equipment,Defect","Ship Staff","Ship Staff Insp.","Topping up air compressor during monthly inspection found the H.P con rod bottom end bearing found to be slack with connecting rod.","E/R - Air Comp.","Emgcy. Systems","Equipment Related","10.32","Very High","","","Informed office, CWP obtained and overhauled and replaced con rod bottom end bearign with both LP and Hp con rod and replaced. Tried out operation satisfactory.","2020-05-10","","Completed","2020-05-10","No","No","No","Internal"]
[null,null,null,null,11831,"54_15-05-2020 17:07:31","2020-05-09","Defect","Ship Staff","Ship Staff Insp.","Funnel damper air actuator found to have air leak and same needs to be overhauled.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.28","Low","","","Funnel damper air actuator renewed with new actuator","2020-06-11","","Completed","2020-05-21","No","No","No","Internal"]
[null,null,null,null,11834,"54_15-05-2020 17:13:51","2020-05-15","Defect","Ship Staff","Ship Staff Insp.","Emergency fire pump compartment drain valve to engine room aft bilge valve is not operational.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.23","Medium","","","The spring loaded valve for emergency fire pump compartment has been overhauled and eased up.","2020-06-08","","Completed","2020-06-13","No","No","No","Internal"]
[null,null,null,null,12127,"54_04/06/2020 6:21:27 PM","2020-05-19","Defect","Ship Staff","Ship Staff Insp.","IG Purge control valve found not operating.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.21","High","","","Spares such as positioner and limit switch box ordered. ( DRED 200123). SPARE RECEIVED JOB IN HAND. job completed on 29-08-2020","2020-09-30","DRED 200123","Completed","2020-08-29","No","No","No","Internal","Spares will be supplied once ready. Target date revised"]
[null,null,null,null,12128,"54_04/06/2020 5:32:00 PM","2020-05-20","Defect","Ship Staff","Ship Staff Insp.","No.2 Control Air Drier found with no gas in the system. ","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","System completely checked and leak test done, freon charged to dryer. Replaced pressure guages. 220 volt low insulation solved, Power switch replaced with toggle switch and now operating satisfactorily.","2020-06-30","","Completed","2020-06-12","No","No","No","Internal"]
[null,null,null,null,12126,"54_04/06/2020 6:15:47 PM","2020-05-25","Defect","Ship Staff","Ship Staff Insp.","No.2 LT Cooler S.W. Inlet valve found not holding .","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Outletr valve sacrificial flange removed and found outlet valve seat ring (Nitrile) damaged/missing of about 50%. Hence outlet valve completely removed and new valve fitted in place with new gaskets. Tested. Found satsifactory.","2020-08-30","","Completed","2020-06-23","No","No","No","Internal","Plan for renewal of valve at load port anchorage."]
[null,null,null,null,12129,"54_04/06/2020 6:09:03 PM","2020-05-30","Critical Equipment","Ship Staff","Ship Staff Insp.","Emergency D/G radiator heater thermostat found defective as temperature found to be not cutting off.","Critical Equip.","Emgcy. Systems","Equipment Related","10.16","Very High","","","Spare thermostat from deep fat fryer was removed and fitted with emergency dg water heater and now made operational.","2020-07-31","","Completed","2020-06-13","No","No","No","Internal"]
[null,null,null,null,12755,"54_09/06/2020 07:42:19 PM","2020-06-02","Defect,Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Slop tank steam heating valve manifold are rusted.To derust and paint.Thinned down valve wheel to renew","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.15","High","","","Derusted and painted.Thinned down valve wheel renewed","2020-07-02","","Completed","2020-07-02","No","No","No","Internal"]
[null,null,null,null,12756,"54_09/06/2020 4:31:29 PM","2020-06-02","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Cave area on 2nd deck needs to arrange","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Cave area arranged. Unwanted debris removed. Items secured.","2020-06-17","","Completed","2020-06-17","No","No","No","Internal"]
[null,null,null,null,12757,"54_09/06/2020 4:33:21 PM","2020-06-02","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Electrical store area on FW expansion tank platform to arrange.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Electrical store items  seggregated and debris removed. Light fittings removed and stored in seperate place.","2020-06-22","","Completed","2020-06-21","No","No","No","Internal"]
[null,null,null,null,12758,"54_09/06/2020 07:23:42 PM","2020-06-02","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Windlass gear case oil indicator is painted green.To clear","Deck - Mooring Machinery","Mooring","Human Error","9.14","Medium","","","Paint cleared and glass cleaned","2020-06-10","","Completed","2020-06-19","No","No","No","Internal","Why Cleaning  glass of gear case pending for so long"]
[null,null,null,null,12759,"54_09/06/2020 07:31:15 PM","2020-06-02","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","In pumproom, various markings from yard is still ther.To paint the affected area","Miscellaneous","Cargo / Ballast Systems","Human Error","8.2","Medium","","","Markings removed and painted.","2020-06-22","","Completed","2020-06-22","No","No","No","Internal"]
[null,null,null,null,12764,"54_09/06/2020 4:14:43 PM","2020-06-02","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Damaged insulation of Cable of sound powered phone in emergency DG room. Cable to renew or new sleeve to use over the existing one.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Cable renewed","2020-06-09","","Completed","2020-06-09","No","No","No","Internal"]
[null,null,null,null,12765,"54_09/06/2020 4:28:37 PM","2020-06-02","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Stbd boiler main steam stop valve lagging is damaged condition. To renew the lagging.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.19","Very High","","","Lagging  renewed.","2020-06-09","","Completed","2020-06-09","No","No","No","Internal"]
[null,null,null,null,12766,"54_09/06/2020 4:06:17 PM","2020-06-02","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Leakage sighted from settling tank filling line flange. TO check and rectify. Lagging to clear off oil","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Observed no oil seepage when transfer pump is running and hence this stain is from previous time. Cleaned and observed no further leakage also lagging cleaned of oil.","2020-06-09","","Completed","2020-06-09","No","No","No","Internal"]
[null,null,null,null,12767,"54_09/06/2020 4:24:11 PM","2020-06-02","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Emergency escape are from bottom platform have rust marks and water marks. ","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.15","Low","","","TP derust patches, chip and paint.","2020-06-17","","Completed","2020-06-15","No","No","No","Internal"]
[null,null,null,null,12768,"54_10/06/2020 02:02:24 PM","2020-06-02","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","In paint locker open eye wash was found.","Miscellaneous","Safety / LSA / FFA","Human Error","8.67","High","","","The eye wash in the paint store was replaced with a new one, officer incharge was instructed to check the eye wash in all locations on a regular basis. The crew were advised to informed HOD and person in charge in case the eyewash is used at any time.","2020-09-01","","Completed","2020-06-06","No","No","No","Internal"]
[null,null,null,null,15614,"54_12/12/2020 12:16:37 PM","2020-06-02","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Engine casing below the new scrubber house needs to derust and paint.","Accommodation","General Appearance","Behaviour Based","10.28","Low","","","Derusting and painting carried out ","2020-07-02","","Completed","2020-06-30","No","No","No","Internal"]
[null,null,null,null,12760,"54_16/06/2020 05:14:46 PM","2020-06-04","Observation","Ship Staff","Ship Staff Insp.","The brake band holding assembly units were found ceased around the hinge pins and joints same to be freed and Greased.","Deck - Mooring Machinery","Mooring","Equipment Related","9.14","Medium","","","Job completed, All brake assemblies derusted, painted, lubricated and fitted.","2020-09-30","","Completed","2020-09-15","No","No","No","Internal"]
[null,null,null,null,12761,"54_16/06/2020 07:42:06 PM","2020-06-04","Defect","Ship Staff","Ship Staff Insp.","No. 7 Mooring winch operating block was seen leaking","Deck - Mooring Machinery","Mooring","Equipment Related","9.14","Medium","","","Renewed the 'o'Ring for the operating block and leak rectified.","2020-06-23","","Completed","2020-07-14","No","No","No","Internal","Do you have  spare O-ring available?"]
[null,null,null,null,12762,"54_16/06/2020 05:09:40 PM","2020-06-12","Defect","Ship Staff","Ship Staff Insp.","The pressure gauge of both Port & Stbd Hose handling cranes were found damaged.","Deck - Machinery","General Appearance","Equipment Related","11.1","High","","","Both hose crane pressure gauges to be renewed","2020-06-23","","Completed","2020-06-22","No","No","No","Internal","Do you have pressure gauge for renewal"]
[null,null,null,null,12763,"54_16/06/2020 1:34:50 PM","2020-06-15","Defect","Ship Staff","Ship Staff Insp.","Garbage compactor pressure switch found to be faulty.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.37","Medium","","","Need to order pressure switch and currently bypassed pressure switch and made operational. RO 200118 raised, supply is awaited.Target date revised.Pressure switch renewed.","2020-11-30","","Completed","2020-10-19","No","No","No","Internal"]
[null,null,null,null,12995,"54_30/06/2020 10:02:07 AM","2020-06-16","Breakdown","Ship Staff","Ship Staff Insp.","Aux Eng -  Oil max filter gear pump seal found leaking during operation.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.28","Low","","","New oil Seals ordered and same to be replaced. Presently oil max unit kept isolated.SPARE RECEIVED JOB IN HAND. pump overhauled, seal renewed","2020-09-15","DRED 200122","Completed","2020-08-21","No","No","No","Internal"]
[null,null,null,null,12996,"54_30/06/2020 9:50:52 AM","2020-06-20","Observation","Ship Staff","Ship Staff Insp.","Galley equipment - (Atta flour mixer) foundation base plate found cracked and vibrates during the operation.","Accommodation","MLC Related","Equipment Related","11.13","Low","","","Equipment shifted to ER Workshop, repaired by strengthening and re-welding by stainless steel material. Same fitted in place and secured.","2020-07-20","","Completed","2020-07-25","No","No","No","Internal"]
[null,null,null,null,13173,"54_12/07/2020 10:13:17 AM","2020-07-01","Defect","Ship Staff","Ship Staff Insp.","One of the ECR Fire door ( Port Side) not closing properly.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.31","Very High","","","Door is slightly bent and full  closure of door is not happening. Few other doors are also in same condition. Defective doors have been identified and office has ordered new doors for fabrication. SPARES RECEIVED, JOB IN HAND. door renewed from spares on 17-08-20","2020-08-30","DRED205073","Completed","2020-08-17","No","No","No","Internal","Understand spares has been received already. What is status."]
[null,null,null,null,13172,"54_07/07/2020 2:49:14 PM","2020-07-02","Observation","Ship Staff","Engineering Audit","ER SPARE PARTS INVENTORY  NOT MAINTAINED AND ITEMS  MISSING FROM STORAGE LOCATION.","E/R - Air Comp.,E/R - Aux. Engine,E/R - Aux. Mach.,E/R - Boiler,E/R - Main Engine,E/R - Pumps,E/R - Purifier,Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.28","Low","","","Spares inventory for M/E, A/E, purifier, Sewage, incinerator, pumps, Air conditioning compressor, Provision compressor completed and updated in PAL.","2020-07-29","","Completed","2020-07-29","No","No","No","Internal"]
[null,null,null,null,13177,"54_06/07/2020 5:47:49 PM","2020-07-04","Defect","Ship Staff","Ship Staff Insp.","Emergency Fire Pump room  drain valve         ( Spring Loaded ) found  hard to operate while pressing the lever\t","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.28","Low","","","Complete valve  removed from place, dismantled,all parts  cleaned and valve seat lapping done. Assembled and fitted in place. Found operating satisfactory.","2020-07-15","","Completed","2020-07-11","No","No","No","Internal"]
[null,null,null,null,13174,"54_06/07/2020 9:19:12 AM","2020-07-06","Critical Equipment","Ship Staff","Ship Staff Insp.","Emergency MDO Pump (Air Driven) found leaking from shaft seal in stopped condition with Suc / Disc valves are open. ","E/R - Aux. Engine","Emgcy. Systems","Equipment Related","10.28","Low","","","To avoid  oil getting collected in save all tray, suction and discharge valves are kept shut. RO to raise for new shaft seal.AWAITING SPARES. Spares received , pump renewed and tried out, satisfactory.","2020-11-30","DRED200146","Completed","2020-11-13","No","No","No","Internal"]
[null,null,null,null,13175,"54_09/07/2020 2:29:56 PM","2020-07-07","Other","Ship Staff","Ship Staff Insp.","Incinerator top side door refractory found damaged in small portion.","Miscellaneous","MARPOL Related","Equipment Related","10.32","Very High","","","Door refractory to be repaired by strengthening with steel mesh wire and using pilibrico material.JOB IN HAND. TARGET DATE REVISED. JOB COMPLETED ","2020-09-15","","Completed","2020-09-02","No","No","No","Internal"]
[null,null,null,null,13176,"54_12/07/2020 10:03:11 AM","2020-07-08","Defect","Ship Staff","Ship Staff Insp.","No.1 Boiler F.O.Pump shaft seal found leaking.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.28","Low","","","Mechanical seal has already been changed. But there is wear on the shaft which needs to be replaced. ROB - Nil.TARGET DATE REVISED mechanical seal, bearings nd gaskets renewed. Pump in use presently without any problems.","2020-11-30","DRED200131","Completed","2020-10-12","No","No","No","Internal"]
[null,null,null,null,13290,"54_24/7/2020 8:21:44 PM","2020-07-23","Defect","Ship Staff","Ship Staff Insp.","No.1 Central F.W. Cooler Plates leak.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.28","Low","","","It was noted the amount of leak between plates in gradually increasing due to defective cooler gaskets. Job to be carreid out at safe anchorage. Vessel has full set of gaskets.JOB IN HAND. TARGET DATE REVISED.JOB COMPLETED. NO LEAKS NOW.","2020-11-30","","Completed","2020-09-24","No","No","No","Internal"]
[null,null,null,null,13291,"54_31/07/2020 9:08:46 AM","2020-07-25","Defect","Ship Staff","Ship Staff Insp.","Elevator car top platform found wet and water seepage inside elevator.","Accommodation","General Appearance","Equipment Related","10.28","Low","","","Duct cover for Elevator natural vent corroded and holed in many places. New cover to be fabricated.As a temperoray measure vent being closed during rain.(Job to be taken up after discharge at Lingii.)JOB IN HAND, TARGET DATE REVISED. JOB COMPLETED","2020-09-20","","Completed","2020-09-19","No","No","No","Internal"]
[null,null,null,null,13292,"54_31/07/2020 9:21:21 AM","2020-07-27","Defect","Ship Staff","Ship Staff Insp.","Prov Crane (Port Side) found with minor leak on the platform.\t","Deck - Machinery","MARPOL Related","Equipment Related","11.1","High","","","Two nos slewing limit valve roller aram found broken and O-ring defective. Roller arm repaired by fabrication but unable to get the correct size Or0ing for sealing. Hence minor leak. RO has been raised for complete limit valve.AWAITING SPARES, TARGET DATE REVISED. RENEWED.","2020-11-30","DRED200150","Completed","2020-10-30","No","No","No","Internal"]
[null,null,null,null,13293,"54_01/08/2020 5:53:23 PM","2020-07-29","Other","Ship Staff","Ship Staff Insp.","Electrical Spare part inventory to take and update in PAL.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.28","Low","","","Electrical Spare part inventory to take and update in PAL.In progress. INVENTORY TAKEN AND UPDATED IN PAL","2020-11-01","","Completed","2020-09-29","No","No","No","Internal"]
[null,null,null,null,21714,"54_22/10/2021 6:39:35 PM","2020-07-31","Observation","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","\n\n1.Mild rust about 2-3 inches long were observed on top two rungs of vertical descending ladder in No 2 port water ballast tank.\n\n2. Two 4 inch long mild rust patch was observed in the inner side and bottom end of deck extension within the no 4 port water ballast tank entrance hatch\n\n","Hull & Tanks","Structural Condn. / WT integrity ","Equipment Related","2.16","Medium","","","Ballast tank entrance tank domes powertooled and painted ","2020-09-29","","Completed","2020-08-11","No","No","No","External"]
[null,null,null,null,13390,"54_01/12/2020 9:15:23 PM","2020-08-10","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Accommodation upper deck port side door rubber packing damaged. Same to renew.     ","Accommodation","Structural Condn. / WT integrity ","Equipment Related","11.6","Medium","","","Accomodation upper deck rubber packing renewed.found in order","2020-08-19","","Completed","2020-08-11","No","No","No","Internal"]
[null,null,null,null,13386,"54_01/12/2020 6:05:23 PM","2020-08-11","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Many of the dresser coupling bolts are corroded and have thinned down. Renew the affected one.","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.5","Medium","","","Renewed the affected ones and replaced with new bolts as required.","2020-12-31","","Completed","2020-12-11","No","No","No","Internal"]
[null,null,null,null,13387,"54_01/12/2020 7:05:23 PM","2020-08-11","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Many of the hydraulic hose end fitting of cranes are not covered with denso tape. Missing one to cover with denso tape after derusting the fitting.     ","Deck - Machinery","Cargo / Ballast Systems","Equipment Related","8.5","Very High","","","Carried out manitennanace of  hydraulic hose end fittings  and other sections  of stbd Midship crane, covered with denso tapes. Maintenance carried out as pr health check report ","2020-12-31","","Completed","2020-12-07","No","No","No","Internal"]
[null,null,null,null,13388,"54_01/12/2020 8:05:23 PM","2020-08-11","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Port side hose handling crane hoisting operation hydraulic hose is damaged and line blanked. New hose already supplier. Renew the hose and check the limits.","Deck - Machinery","Cargo / Ballast Systems","Equipment Related","8.5","Very High","","","Hydraulic hose renewed. Need to be function tested.JOB COMPLETED","2020-08-18","","Completed","2020-08-13","No","No","No","Internal"]
[null,null,null,null,13389,"54_01/12/2020 9:05:23 PM","2020-08-11","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Oil leak sighted below the operating block of MW 6 A . Source to find and rectify.","Deck - Mooring Machinery","Mooring","Equipment Related","9.14","Medium","","","Oil leak arrested by maintenance on the operating block of MW 6A, O ring renewed.","2020-08-30","","Completed","2020-08-12","No","No","No","Internal"]
[null,null,null,null,13391,"54_01/12/2020 10:05:23 PM","2020-08-11","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","In steering Gear room, 3 of the pressure flanges of the mooring winch line has drop leak. O-ring to change.","Deck - Mooring Machinery","Eng. / Strg. Comp.","Equipment Related","10.28","Low","","","o-rings already onboard kept in store near workshop and same needs to be replaced.FLANGES TIGHTENED. BOLTS FOUND SLIGHTLY SLACK. LEAK HAS STOPPED.","2020-09-30","","Completed","2020-09-26","No","No","No","Internal"]
[null,null,null,null,13392,"54_01/12/2020 11:05:23 PM","2020-08-11","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Air dryer no 2 is reported to have leak in refrigerant line. To pinpoint the leak and rectify.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.28","Low","","","To identify leak and rectify. LEAK FOUND AND RECTIFIED. SYSTEM IN OPERATION FOR ALMOST TWO WEEKS.","2020-09-30","","Completed","2020-09-03","No","No","No","Internal","When is job planned for?"]
[null,null,null,null,13393,"54_01/12/2020 9:45:23 PM","2020-08-11","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Incinerator panel touch screen is very blurred. To replace.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Panel renewed upon receipt.","2020-11-30","DRED200155","Completed","2020-11-09","No","No","No","Internal"]
[null,null,null,null,13858,"54_04/09/2020 05:05:43 PM","2020-08-30","Other","Ship Staff","Ship Staff Insp.","Hydraulic line of Valve remote conrol system on deck found modertae to heavily corroded on main deck aft of the manifold.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.15","High","","","Derusting and painting of VRCS main line from midship to aft  including pipeline and U clamps area carried out by removing the U clamps, Renewed return line pipe for Box no.4. All branch line and main line covered","2020-10-30","","Completed","2020-10-01","No","No","No","Internal"]
[null,null,null,null,13859,"54_04/09/2020 05:14:57 PM","2020-08-31","Other","Ship Staff","Ship Staff Insp.","Hydraulic line for mooring system on main deck at forward Branch libe leading to mooring winch M5 found modertae to heavy corroded at 02 location, Areas marked and located.","Deck - Mooring Machinery,Deck - Pipe / Fittings","Mooring","Equipment Related","8.15","High","","","Derusting and painting of Mooring main  line from midship to aft  including pipeline and U clamps area carried out, Renewal of Pipeline carried out for MW 4A. ","2020-10-31","","Completed","2020-10-14","No","No","No","Internal"]
[null,null,null,null,13979,"54_16/09/2020 04:06:03 AM","2020-09-09","Non Conformity,Observation","Ship Staff","Ship Staff Insp.","LUGS ARE NOT  FITTED  FOR DIFFERENT FREE BOARDS  FOR RIGGING PILOT LADDER","Deck - Pipe / Fittings","Safety / LSA / FFA","Equipment Related","5.47","Medium","","","TO FARICATE AND WELD THE LUGS ON MAIN DECK NEAR THE GANGWWAY PORT & STBD. job moved to refamna and intended to be completed in upcoming DD.","2021-06-15","","Completed","2021-04-07","No","No","No","Internal","Repair to be carried out in ballast passage."]
[null,null,null,null,13983,"54_15/09/2020 9:54:41 AM","2020-09-14","Defect","Ship Staff","Ship Staff Insp.","SOOT TANK EDUCTOR FOUND WASTED AND WITH MULTIPLE PIN HOLES","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.31","Very High","","","RO 200162 RAISED FOR NEW EDUCTOR.TEMPORARY COLD REPAIR DONE. WELDING REPAIR DONE. TRIED OUT. AGAIN MULTIPLE PINHOLES DEVELOPED OVER LARGE AREA. INTEND TO MAKE COMBINATION OF WELDING AND COLD REPAIR FOR USE UNTIL NEW SPARE IS RECEIVED. Spare renewed upon receipt.","2020-12-31","DRED 200162","Completed","2020-11-08","No","No","No","Internal","Repair it by welding."]
[null,null,null,null,13984,"54_15/09/2020 10:52:15 AM","2020-09-14","Defect","Ship Staff","Ship Staff Insp.","FWD MOORING WINCH MW1A DRUM FOUND WITH MINOR WOBBLE.SUSPECT BEARING WORN OUT","Deck - Mooring Machinery","Mooring","Equipment Related","9.2","Very High","","","SLEEVE BEARING TO BE RENEWED IN DRYDOCK. PROPER GREASING TO BE ENSURED AT ALL TIMES. JOB TRANSFERRED TO REFMAN.","2021-10-31","","Completed","2021-04-06","Yes","No","No","Internal","Does vessel have spare bearing?"]
[null,null,null,null,13985,"54_16/09/2020 12:59:58 AM","2020-09-14","Other","Ship Staff","Ship Staff Insp.","AUS suc pressure guage , No.2 Aus flow control valve indication , No.2 cargo eductor suc gauge, ballast eductor suction gauge showing erratic reading","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.23","Medium","","","Caliberation carried out fro the pressure guages for , No.2 Aus flow control valve indication , No.2 cargo eductor suc gauge, ballast eductor suction gauge , Stataus of Aus and No.2 Cargo eductor guages to be checked during discharging. No.2 Ballast eductor showing erratic reading. ALL GUAGES CALIBRATED AND CHECKED DURING DISCHARGING.FOUND WORKING IN GOOD ORDER.","2020-10-31","","Completed","2020-10-15","No","No","No","Internal"]
[null,null,null,null,14887,"54_04/11/2020 11:57:47 AM","2020-10-14","Other","Ship Staff","Ship Staff Insp.","The thermal printer for anemometer MODEL : AP-P 40, DWG NO:DIC AZ 10009, found unoperational, Upon opening the unit  observed damage to the drum. ","Miscellaneous","Cargo / Ballast Systems","Equipment Related","8.1","Very High","","","Requisition raised for the new printer ref:DRED200225. Supplied and installed.","2021-03-28","DRED200225","Completed","2021-03-01","No","No","No","Internal"]
[null,null,null,null,14889,"54_04/11/2020 12:02:05 PM","2020-10-26","Defect","Ship Staff","Ship Staff Insp.","SLOP-P  IG branch valve found passing (not holding) While carrying out safety rounds at sea.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.22","Very High","","","Received new seat ring and renewed the seat ring of Slop-P valve, The disc of the valve also found erroded at the circumference, new disc fitted from a spare valve, no more leak.To raise requisition for spare valave (with valve disc)","2020-11-20","","Completed","2020-11-10","No","No","No","Internal"]
[null,null,null,null,14890,"54_15/11/2020 9:39:21 PM","2020-11-02","Observation","Ship Staff","Ship Staff Insp.","Chipping and painting of soot tank to be carried out.","Hull & Tanks","Eng. / Strg. Comp.","Equipment Related","10.28","Low","","","Tank internally chipped and painted.","2020-11-15","","Completed","2020-11-13","No","No","No","Internal"]
[null,null,null,null,14888,"54_16/11/2020 02:47:52 PM","2020-11-10","Defect","Ship Staff","Ship Staff Insp.","The remote sounding of 1P,1S & 3S WBT showing erratic readings","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.13","Medium","","","The same has been serviced by HKT marine and still  has deviation of 35  cm. 1S and 3S sensor replaced. 1P only serviced.","2021-05-10","DRED210053","Completed","2021-05-10","No","No","No","Internal"]
[null,null,null,null,15613,"54_15/12/2020 08:59:50 AM","2020-12-11","Other","Ship Staff","Ship Staff Insp.","Minor seepage observed from shaft seal of Mooring Winch MW1 & MW3","Deck - Mooring Machinery","Mooring","Equipment Related","9.14","Medium","","","MW-1 and MW-3 gearcase V packing was suspected weeping. When the cover was dismantled it was found that there is no packing at the leak location- instead it is miniscule amounts of melted grease from the roller bearing which shows as a slight stain. No further action required for this. ","2021-01-31","","Completed","2021-02-04","No","No","No","Internal"]
[null,null,null,null,19346,"54_04/05/2021 11:40:00 AM","2021-02-09","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Elevator T cable to be renewed.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","T Cable renewed with new spare recieved under RO DRED210055","2021-07-31","DRED210055","Completed","2021-07-28","No","No","No","Internal","T-cable has been ordered and will be replaced this call Singapore during annual Survey."]
[null,null,null,null,19347,"54_04/05/2021 11:30:26 AM","2021-02-09","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Various insulation matts missing infront of Panels in  Scrubber room ","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Human Error","10.24","Low","","","Missing insulation matts installed in place.","2021-02-25","","Completed","2021-02-14","No","No","No","Internal"]
[null,null,null,null,19348,"54_04/05/2021 11:35:35 AM","2021-02-09","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Main engine exhaust pipe aft of EGB drain valve to be blanked","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Valve blanked.","2021-02-11","","Completed","2021-02-10","No","No","No","Internal"]
[null,null,null,null,19349,"54_04/05/2021 11:47:25 AM","2021-02-09","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","EGCS deck house portable fire extinguishers monthly checks not done since July 2020.","LSA / FFA","Eng. / Strg. Comp.","Human Error","8.71","Very High","","","Upon sighting observation the inspection was carried out immidiately and all found in order","2021-02-10","","Completed","2021-02-09","No","No","No","Internal"]
[null,null,null,null,19350,"54_04/05/2021 11:50:18 AM","2021-02-09","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Main deck P& S gutter plate to derust and paint","Deck - Machinery,Deck - Mooring Machinery","Eng. / Strg. Comp.","Equipment Related","11.3","Medium","","","Main Deck P& S gutter plate derusted and painted.","2021-05-09","","Completed","2021-05-04","No","No","No","Internal"]
[null,null,null,null,18075,"54_27/2/2021 1:41:40 PM","2021-02-09","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Pump room flashing horn not operational","Deck - Machinery","Communication","Equipment Related","8.48","Medium","","","Renewed with new Spare. New base plate fabricated and fitted inplace","2021-08-25","DRED210056","Completed","2021-08-04","No","No","No","Internal","Spare on order and will be supplied once ready."]
[null,null,null,null,18080,"54_27/2/2021 1:16:05 PM","2021-02-09","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Port windlass gear oil contaminated with water.","Deck - Machinery","Mooring","Equipment Related","9.2","Very High","","","Gear oil replenished with new oil, possible water ingress areas covered when system not in use.","2021-02-28","","Completed","2021-02-26","No","No","No","Internal"]
[null,null,null,null,21715,"54_22/10/2021 6:33:10 PM","2021-02-09","Observation","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","Vessel was noted with old edition (2011) Code of Safe Working Practiced in use in the vessel CCR.","Miscellaneous","Cert. & Docu.","Human Error","8.1","Very High","","","Code of Safe working practices was replaced with 2015 addition with 2020 amendments at Singapore on 09 Feb 21 during bunkering ","2021-05-09","","Completed","2021-02-10","No","No","No","External"]
[null,null,null,null,18073,"54_27/2/2021 1:22:02 PM","2021-02-10","Defect,Guarantee Claim","Ship Staff","Ship Staff Insp.","BWTS system valve FCV1211 not operational in auto mode, Filter fault alarm active with the system.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","6.21","High","","","PCB to be changed as per maker mail GC rasied from vessel end for the same. Filter fault alarm in communication with maker. GC index maintained seperately and same closed in DDRL","2021-07-22","","Completed","2021-06-16","No","No","No","Internal"]
[null,null,null,null,18074,"54_27/2/2021 1:34:17 PM","2021-02-10","Defect","Ship Staff","Ship Staff Insp.","High sea chest MGPS Aluminium anode alarm","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.37","Medium","","","New MGPS Cabinet received, fitted and alarm cleared now.","2021-06-29","DRED210032","Completed","2021-04-26","No","No","No","Internal"]
[null,null,null,null,18078,"54_12/02/2021 4:10:55 PM","2021-02-10","Breakdown","Ship Staff","Ship Staff Insp.","Electric motor to be replaced\t","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.37","Medium","","","New electric motor fitted in place.","2021-02-13","DRED210054","Completed","2021-02-11","No","No","No","Internal"]
[null,null,null,null,18079,"54_27/2/2021 1:08:56 PM","2021-02-10","Breakdown","Ship Staff","Ship Staff Insp.","Steering gear grease pump not operational same to be replaced upon receiving spare.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Steering gear grease pump replaced with spare received","2021-02-27","DRED200167","Completed","2021-02-22","No","No","No","Internal"]
[null,null,null,null,18081,"54_27/2/2021 1:32:00 PM","2021-02-10","Defect","Ship Staff","Ship Staff Insp.","LGSP 7 Forward insulation meter faulty","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","LGSP7 forward insulation meter replaced with spare received.","2021-02-28","DRED200085","Completed","2021-02-24","No","No","No","Internal"]
[null,null,null,null,18076,"54_12/02/2021 5:31:16 PM","2021-02-12","Breakdown,Defect","Ship Staff","Ship Staff Insp.","TWO chemical dosing pumps – one for No.2 boiler and one for HP drum are not working( pumping).","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Pump overhauled and  operational but performance lower compared to other pumps with same setting. As of now it is pumping and we will also receive spare pump.","2021-06-12","DRED 210014","Completed","2021-03-09","No","No","No","Internal"]
[null,null,null,null,18082,"54_27/2/2021 1:00:49 PM","2021-02-14","Defect","Ship Staff","Ship Staff Insp.","Aux DG water washing lines clogged","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Aux DG water washing lines removed chockage cleared and put back in use.","2021-02-28","","Completed","2021-02-16","No","No","No","Internal"]
[null,null,null,null,18077,"54_27/2/2021 12:56:25 PM","2021-02-16","Defect","Ship Staff","Ship Staff Insp.","ICO lube sample oil pump alarms","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","SO Pump Stator replaced with new spare recieved under RO DRED215094. Tried out system working satisfactorily without any alarms","2021-07-20","DRED215094","Completed","2021-07-30","No","No","No","Internal","Pump rotor is on order and have lead time. will be connected this call Singapore. Target date revised. PO no is DRED215094"]
[null,null,null,null,18083,"54_27/2/2021 1:26:41 PM","2021-02-18","Defect","Ship Staff","Ship Staff Insp.","MW8 and MW10 relief line unions found leaking","Deck - Mooring Machinery,Deck - Pipe / Fittings","Mooring","Equipment Related","9.14","Medium","","","MW8 and MW10 relief line unions found leaking and same renewd with available spare union and leak arrested.","2021-02-28","","Completed","2021-02-25","No","No","No","Internal"]
[null,null,null,null,18072,"54_27/2/2021 12:54:04 PM","2021-02-26","Defect","Ship Staff","Ship Staff Insp.","No 2 control air dryer out of operation","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Control Air dryer compressor thermostat was replaced by new spare. Evaporator coil was fully coated with oil same cleaned. condensor cleaned and put in operation and now operational without issues.","2021-04-15","","Completed","2021-03-05","No","No","No","Internal"]
[null,null,null,null,18451,"54_01/04/2021 6:41:05 PM","2021-02-27","Other","Ship Staff","Ship Staff Insp.","Fresh Water Tank Port Discharge Valve not holding/ Leaking\t\t","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Valve repalced with new spare available onbaord while tank empited for cleaning.","2021-05-29","","Completed","2021-03-29","No","No","No","Internal"]
[null,null,null,null,18442,"54_01/04/2021 6:31:31 PM","2021-03-01","Other","Ship Staff","Ship Staff Insp.","FW Hyrophore Both Pumps Discharge Valve not holding","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Valves received and renewed.","2021-05-31","DRED210065","Completed","2021-05-28","No","No","No","Internal"]
[null,null,null,null,18452,"54_01/04/2021 5:49:32 PM","2021-03-01","Other","Ship Staff","Ship Staff Insp.","Aux Boiler # 1 FD Fan Outlet bellow Torn/cracked.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.3","Medium","","","Expansions bellow replaced with new spare bellow available onbaord.","2021-03-15","","Completed","2021-03-10","No","No","No","Internal"]
[null,null,null,null,18453,"54_01/04/2021 6:20:17 PM","2021-03-01","Other","Ship Staff","Ship Staff Insp.","Aux Boiler # 2 Inlet bellow to furnance crack/torn\t","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Expansion Bellow replaced with spare new available onboard","2021-03-15","","Completed","2021-03-09","No","No","No","Internal"]
[null,null,null,null,18220,"54_14/3/2021 12:39:12 PM","2021-03-04","Other","Ship Staff","Ship Staff Insp.","One Section of Galley Drain overboard Pipe Pin Holed","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.3","Medium","","","Section Removed, Lekaage Rectifed by welding the pipe section.","2021-03-15","","Completed","2021-03-09","No","No","No","Internal"]
[null,null,null,null,18218,"54_14/3/2021 12:48:03 PM","2021-03-05","Other","Ship Staff","Ship Staff Insp.","Incinerator Waste Oil Service Tank heating condnesate drain line one section flange gasket leaking.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Gasket renewed and stema leak rectified after isolating steam plant","2021-03-18","","Completed","2021-03-11","No","No","No","Internal"]
[null,null,null,null,18219,"54_14/3/2021 12:57:23 PM","2021-03-05","Other","Ship Staff","Ship Staff Insp.","ECO feed pump # 2 Motor Making Abnormal sound and vibration","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.3","Medium","","","Motor overhauled, Bearing reneewed, Motor Coupling Bolts renewed with new spare.","2021-03-30","","Completed","2021-03-12","No","No","No","Internal"]
[null,null,null,null,18990,"54_23/04/2021 5:13:07 PM","2021-03-11","Defect","Ship Staff","Ship Staff Insp.","Boiler salinometer Defective","E/R - Boiler,E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Boiler salinometer replaced with available spare onboard and now operational and in order.","2021-05-07","","Completed","2021-04-12","No","No","No","Internal"]
[null,null,null,null,18217,"54_14/3/2021 12:43:20 PM","2021-03-12","Defect","Ship Staff","Ship Staff Insp.","Aux Boiler # 1 And # 2 Exhaust Uptake Expanbison Bellows Cracked and leaking","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","New Bellows ordered and fitted in Drydock. Job in REFMAN and same completed here.","2021-06-30","","Completed","2021-04-06","Yes","No","No","Internal"]
[null,null,null,null,18454,"54_01/04/2021 6:48:09 PM","2021-03-15","Other","Ship Staff","Ship Staff Insp.","Tracing steam line for ME FO near mano platform # 3 unit leaking","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Leak rectifed by renewing the connection","2021-03-30","","Completed","2021-03-19","No","No","No","Internal"]
[null,null,null,null,18455,"54_01/04/2021 7:11:06 PM","2021-03-15","Other","Ship Staff","Ship Staff Insp.","TG Condensate drain pot Condensate drain line above TG Vacuum Condenser near ship side leaking\t","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Leakage rectified after isolating TG system, by renewing the gasket of leaking flange.","2021-03-31","","Completed","2021-03-24","No","No","No","Internal"]
[null,null,null,null,18456,"54_01/04/2021 6:22:55 PM","2021-03-17","Other","Ship Staff","Ship Staff Insp.","Aux Boiler  # 1 Inlet bellow to furnance found damaged/leaking\t","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Expansion Bellow renewed with new spare available onboard","2021-03-21","","Completed","2021-03-20","No","No","No","Internal"]
[null,null,null,null,18443,"54_02/04/2021 12:53:35 PM","2021-03-24","Defect,Guarantee Claim","Ship Staff","Ship Staff Insp.","BWTS - TRO Sensor AIT-151 & AIT-251 box does not seal properly. \n\nAIT-151 is not switching over to Safe operation mode even after pushing the door shut. AIT-251 also has the same issue but is less persistant than AIT-151.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","6.21","High","","","Air from box found to be leaking in electrical cable glands and same arrested and now in order.","2021-04-30","","Completed","2021-04-06","No","No","No","Internal"]
[null,null,null,null,18444,"54_02/04/2021 01:20:01 PM","2021-03-24","Defect,Guarantee Claim","Ship Staff","Ship Staff Insp.","BWTS - SAMPLE WATER FLOW CONTROL METERING VALVE                                               Metering Valves to control flow and by pass sample flow to TRO Sensor AIT-151 & AIT-251 have been found to be off set and slipping during operation. ","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","6.21","High","","","Metering valve received. Also Gc defects for BWTS maintained in seperate index.","2021-04-30","","Completed","2021-06-01","No","No","No","Internal"]
[null,null,null,null,18445,"54_02/04/2021 01:23:40 PM","2021-03-24","Guarantee Claim","Ship Staff","Ship Staff Insp.","BWTS - TE-1111 FEED WATER TEMP SENSORHIGH LEVEL ALARM WAS BEING DISPLAYED, BECAUSE OF WHICH SEQUENCE FOR BALLASTING WERE UNSUCCESSFUL. NO CHANGE IN DISPLAYED VALUE AFTER STOPPING OPERATIONS. SUSPECT SENSOR FAILURE IN THE SAME. ","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","6.21","High","","","GC received. Installed and now operational.","2021-04-30","","Completed","2021-05-04","No","No","No","Internal"]
[null,null,null,null,18446,"54_02/04/2021 01:30:11 PM","2021-03-24","Guarantee Claim","Ship Staff","Ship Staff Insp.","BWTS - SOLENOID VALVE XV 2511 INTERMITTENT FAILUREDURING BALLASTING OPERATION PREVENTING FLOW OF WATER TO TRO SENSOR, SUSPECTED SIGNAL FAILURE TO VALVE AT TIME OF OPERATION.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","6.21","High","","","GC Spare part received in DD","2021-04-30","","Completed","2021-05-04","No","No","No","Internal"]
[null,null,null,null,18447,"54_02/04/2021 01:41:40 PM","2021-03-24","Defect","Ship Staff","Ship Staff Insp.","REMOTE GAUGING SYSTEM OF 4 P WBT SHOWING ERRATIC READINGS","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.13","Medium","","","Same was service by HKT marine and replaced 4 Port sensor and however has ana error of 35 cms.","2021-04-30","","Completed","2021-05-10","No","No","No","Internal"]
[null,null,null,null,18450,"54_02/04/2021 12:44:09 PM","2021-03-24","Defect,Guarantee Claim","Ship Staff","Ship Staff Insp.","BWTS FLOWMETER FLOWMETER FIT - 1211 - Giving Readings Much Higher Than The Rated Capacity of the Ballast Pump. As a result if the rate is not brought down the Rectifier's trip during Ballasting. During Deballasting also the same has been noticed that the rate displayed was close to 4700 m3/hr though the Pumps capacity is 3000 m3/hr.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","6.21","High","","","Makers have been informed. Guarantee Claim have been raised for same.  Job Closed as per super mail on 01-06-2021. BWTS GC maintained in seperate index.","2021-04-30","","Completed","2021-06-01","No","No","No","Internal"]
[null,null,null,null,18448,"54_2/4/2021 3:16:53 PM","2021-03-25","Defect","Ship Staff","Ship Staff Insp.","In EGCS S.W pump outlet manifold, weld connection inlet to water analyser unit has pin hole.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Pin hole is temporarily repaired by screwing screw Pin hole welded and repaired permanently in DD.","2021-05-28","","Completed","2021-04-29","No","No","No","Internal"]
[null,null,null,null,18449,"54_2/4/2021 3:25:08 PM","2021-03-25","Defect","Ship Staff","Ship Staff Insp.","Port side provision crane hydraulic luffing cylinder oring in bottom has minor seepage.","Deck - Machinery","Structural Condn. / WT integrity ","Equipment Related","8.5","Very High","","","Luffing cylinder overhauled in DD by yard with new seals and now in order.","2021-06-20","","Completed","2021-05-11","Yes","No","No","Internal"]
[null,null,null,null,18457,"54_01/04/2021 6:26:23 PM","2021-03-25","Other","Ship Staff","Ship Staff Insp.","Aft Hyd Cooler SW Inlet Pipe section after inlet valve found pin holed and leaking","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Pipe Section renewed with new pipe and flange","2021-03-30","","Completed","2021-03-27","No","No","No","Internal"]
[null,null,null,null,21716,"54_22/10/2021 6:23:54 PM","2021-04-15","Observation","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","VIQ 10.8\n\n Bunker Checklist dated 10/August/2020 did not confirm whether vessel had received the MSDS (item  21 and 22)\n\nBunkering checklists were in use since August 2020 had missing space between the words in some of the checkpoints, difficult to understand those unspaced texts and sentences\n\n","Miscellaneous","Cert. & Docu.","Human Error","10.8","Medium","","","Master Briefed all Crew on correct procedures of filling bunker checklists as per ISGOTT ","2021-04-30","","Completed","2021-04-26","No","No","No","External"]
[null,null,null,null,19526,"54_15/05/2021 12:58:19 PM","2021-05-14","Defect","Ship Staff","Ship Staff Insp.","DG FO Auto back wash filter GC55 unit found to be faulty.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Replaced with new Spare received. Setting checked and made same. Working satsiafactory.","2021-08-15","DRED210100","Completed","2021-08-04","No","No","No","Internal","Spare on order and will be supplied once ready."]
[null,null,null,null,19547,"54_31/05/2021 11:03:57 AM","2021-05-16","Defect","Ship Staff","Ship Staff Insp.","HFO purifier # 1 3 way circualtion valve leaking from tele tele hole","E/R - Purifier","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","RO raised for spares. Spare received, will be attempting after discharging. Running, under observation, no leak at present. Both purifiers also run in parallel for 9 hours- no leaks observed.","2021-09-30","DRED 210090","Completed","2021-09-16","No","No","No","Internal","Sapres already supplied."]
[null,null,null,null,19548,"54_31/05/2021 3:52:51 PM","2021-05-16","Defect,Observation","Ship Staff","Ship Staff Insp.","Funnel for Air cooler condensate drain pot For all 3 DG Found rusted and wasted","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","New funnel fabricated, painted and Fixed in place.","2021-06-30","","Completed","2021-06-02","No","No","No","Internal"]
[null,null,null,null,19546,"54_31/05/2021 10:35:58 AM","2021-05-17","Defect","Ship Staff","Ship Staff Insp.","Vent valve for IGS found not Working in auto.","Inert Gas","Eng. / Strg. Comp.","Equipment Related","8.25","Very High","","","Repalced with new spare receieved. Tried out working satisfactorily.","2021-08-17","DRED210069","Completed","2021-08-04","No","No","No","Internal","Spare on order and will be supplied once ready."]
[null,null,null,null,19549,"54_31/05/2021 3:49:29 PM","2021-05-18","Defect","Ship Staff","Ship Staff Insp.","LT Cooler drain scupper pipe clogged and choked","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Section wise pipe removed and all the pipes cleared.","2021-06-30","","Completed","2021-06-01","No","No","No","Internal"]
[null,null,null,null,19551,"54_31/05/2021 3:45:04 PM","2021-05-25","Defect","Ship Staff","Ship Staff Insp.","Cascade tank drain scupper pipe found choked.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Various pipe sections removed and line cleared.","2021-06-30","","Completed","2021-05-29","No","No","No","Internal"]
[null,null,null,null,19550,"54_01/06/2021 12:18:35 AM","2021-05-28","Other","Owner / Marine / Tech. Suptd.","Onboard Training","Engineering Campaign 02 of 2021 compliance","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Knowledge Based","","","","","To complete vessel action in Engineering campaign 02 of 2021.","2021-06-28","","Completed","2021-06-28","No","No","No","Internal"]
[null,null,null,null,19700,"54_05/06/2021 12:06:22 PM","2021-06-01","Defect","Ship Staff","Ship Staff Insp.","FWG Save all tray drain Scupper pipe clogged","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","6 pipe sections remeoved and all new sections fabricated, painted and put in place.","2021-06-30","","Completed","2021-06-16","No","No","No","Internal"]
[null,null,null,null,19701,"54_02/06/2021 5:24:36 PM","2021-06-01","Defect","Ship Staff","Ship Staff Insp.","ME FO Heater # 2 Steam outlet flange leaking\t","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Gasket for flange to renewed","2021-06-30","","Completed","2021-06-15","No","No","No","Internal"]
[null,null,null,null,19702,"54_15/06/2021 7:03:34 PM","2021-06-02","Defect","Ship Staff","Ship Staff Insp.","During weekly maintenance notice one of the batteires of port Lifeboat is showing renewal indication","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.29","High","","","Lifeboat batteries repalced with new spare received","2021-07-30","DRED210115","Completed","2021-07-30","No","No","No","Internal","Replacement will be supplied this call Singapore."]
[null,null,null,null,19703,"54_02/06/2021 5:21:45 PM","2021-06-02","Defect,Observation","Ship Staff","Ship Staff Insp.","ME 2 units Flexible hoses for ICU having seepage/slight lekage","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","ICU hoses renewed with available spare onboard.","2021-06-30","","Completed","2021-06-11","No","No","No","Internal"]
[null,null,null,null,19842,"54_29/06/2021 12:50:06 AM","2021-06-20","Defect,Observation","Ship Staff","Ship Staff Insp.","LP TEMP PROBE 12 HIGH TEMP SENSOR FAILURE","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","SENSOR TO RENEW WITH NEW SENSOR AT DISCHARGE PORT ONSAN","2021-07-31","","Completed","2021-07-17","No","No","No","Internal","Does vessel have spare sensor?"]
[null,null,null,null,22223,"54_26/10/2021 10:26:50 AM","2021-06-26","Observation","Owner / Marine / Tech. Suptd.","ISM Audit","ISM: Environmental Seal log Deck seals were not updated correctly","Documentation","ISM Related","Inappropriate Procedure","6.4","High","","","Seal log checked physically and input the correct seal in places","2021-09-26","","Completed","2021-08-27","No","No","No","Internal"]
[null,null,null,null,22224,"54_26/10/2021 10:32:13 AM","2021-06-26","Observation","Owner / Marine / Tech. Suptd.","ISM Audit","ISM: Engineers not familiar with Data retrieval procedure from OWS","Miscellaneous","ISM Related","Knowledge Based","6.17","Very High","","","Data retrieved practically from OWS and all engineers trained.","2021-09-26","","Completed","2021-08-27","No","No","No","Internal"]
[null,null,null,null,19839,"54_30/06/2021 03:01:31 PM","2021-06-28","Defect,Observation","Ship Staff","Ship Staff Insp.","Fireman Suit (3 Nos) Pant frayed at bottom","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.43","High","","","Vessel carried out stitching at the torn part as per office instructions. insulation is in good order.","2021-08-15","","Completed","2021-07-07","No","No","No","Internal"]
[null,null,null,null,19840,"54_30/06/2021 03:04:51 PM","2021-06-28","Defect","Ship Staff","Ship Staff Insp.","In Stbd side pilot ladder, one step is repaired and one spreader is repaired  showing signs of cracking up.","Miscellaneous","Safety / LSA / FFA","Equipment Related","5.47","Medium","","","NEW PILOT LADDER received at singapore and replaced.","2021-08-15","DRED210130","Completed","2021-07-31","No","No","No","Internal","New pilot ladder will be supplied in this call Singapore."]
[null,null,null,null,19841,"54_30/06/2021 03:12:36 PM","2021-06-28","Defect","Ship Staff","Ship Staff Insp.","BHC test kit found leaking and unusable","Miscellaneous","Mooring","Equipment Related","9.7","Medium","","","Spares received and overhauled.","2021-08-15","DRED215089","Completed","2021-07-30","No","No","No","Internal","Spare on order and will be supplied once ready."]
[null,null,null,null,19845,"54_30/06/2021 07:24:53 PM","2021-06-28","Defect","Ship Staff","Ship Staff Insp.","Hydroblaster found leaking from several parts including dump gun , booster pump , hoses.Noticed Main pump push coupling fittings missing and PU hoses were broken.Filter unit found to be missing,pump casing securing stud 2 nos broken.","Miscellaneous","General Appearance","Equipment Related","11.1","High","","","vessel has ordered various spare parts under requisition no.DRED210093. Vessel will order remaning spare parts in due time under different requisition. Another hydroblaster received, now one machine working well and in use.","2021-08-31","DRED210093","Completed","2021-08-27","No","No","No","Internal","Since new pump has been supplied. Shwo this as completed."]
[null,null,null,null,20072,"54_15/07/2021 1:10:20 PM","2021-07-01","Defect,Observation","Ship Staff","Ship Staff Insp.","ME FWD Air Cooler Feed water heater inlet pipe having Pin hole near the safety valve flange","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.3","Medium","","","After Arrival drifting, Pipe removed from place and permanent repairs carried out by taking the pipe to workshop.","2021-07-15","","Completed","2021-07-14","No","No","No","Internal"]
[null,null,null,null,20071,"54_15/07/2021 1:28:53 PM","2021-07-02","Breakdown","Ship Staff","Ship Staff Insp.","No.2 Main Air Compressor Motor Giving Low Insualtion. Found one Winding Damaged.","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related","10.3","Medium","","","Installed new motor. Tried out working satsifactorily","2021-08-31","DRED215098","Completed","2021-08-02","No","No","No","Internal","Spare motor will be supplied in this call Singapore."]
[null,null,null,null,20073,"54_15/07/2021 1:16:53 PM","2021-07-02","Other","Ship Staff","Ship Staff Insp.","ME Aft Cooler drain orifice choked\t","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.3","Medium","","","After Arrival drifting at dis port, pipe and orifice reomved from place cleaned and de rusted","2021-07-17","","Completed","2021-07-14","No","No","No","Internal"]
[null,null,null,null,20074,"54_15/07/2021 1:33:24 PM","2021-07-03","Defect,Observation","Ship Staff","Ship Staff Insp.","ME # 1 and # 6 unit ICU return servo flexible hose leaking","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.3","Medium","","","Flexible hose along with ball valve replaced with new spare avaiblae onbaord","2021-07-17","","Completed","2021-07-14","No","No","No","Internal"]
[null,null,null,null,20075,"54_15/07/2021 1:39:56 PM","2021-07-03","Defect,Observation","Ship Staff","Ship Staff Insp.","Provision crane port side found oil seepage through limit switch block","Deck - Machinery","Structural Condn. / WT integrity ","Equipment Related","8.5","Very High","","","Leakge rectified by renewing all o-rings of limit switch ","2021-07-15","","Completed","2021-07-13","No","No","No","Internal"]
[null,null,null,null,20238,"54_31/07/2021 2:32:52 PM","2021-07-25","Observation","Ship Staff","Suptd. Insp.","Emergency Escape Drain pipe choke to clear","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Pipe section removed and cleared.","2021-08-07","","Completed","2021-08-02","No","No","No","Internal"]
[null,null,null,null,20264,"54_31/07/2021 2:36:33 PM","2021-07-27","Observation","Ship Staff","Ship Staff Insp.","Drain TG vacuum condensor pipe choke","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.3","Medium","","","Pipe sections removed and all blockages cleared.","2021-08-09","","Completed","2021-07-31","No","No","No","Internal"]
[null,null,null,null,22225,"54_26/10/2021 4:11:04 PM","2021-07-28","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","M/E PERFORMANCE TO BE MARKEDON PROPELLER CURVE ANS SAME TO BE FILED ALONGWITH SEEMP FILE EVERY 6 MONTHS","Documentation","Eng. / Strg. Comp.","Inappropriate Procedure","","","","","PROPELLER CURVE TO BE PLOTTED EACH TIME PERFORMANCE IS TAKEN.","2021-09-28","","Completed","2021-09-02","No","No","No","Internal"]
[null,null,null,null,20237,"54_31/07/2021 1:39:22 PM","2021-07-29","Defect,Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Both windlass hydraulic brake to set again and same not matching with marking.","Deck - Mooring Machinery","Mooring","Equipment Related","9.2","Very High","","","Brake of port and starboard anchor adjusted to correct marking on the plate","2021-08-05","","Completed","2021-08-02","No","No","No","Internal"]
[null,null,null,null,20239,"54_31/07/2021 1:45:47 PM","2021-07-29","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","4 boxes of Cooler gasket  are stored on top of the air con blower unit in air con room. Same to be removed and store properly.","Miscellaneous","General Appearance","Equipment Related","11.13","Low","","","To stack properly and secured with wire rope.","2021-08-22","","Completed","2021-08-28","No","No","No","Internal","Why is it pending for so long? IT will hardly take 2 hour."]
[null,null,null,null,20240,"54_31/07/2021 1:50:05 PM","2021-07-29","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Insulation mat at various places in engine room are not in good condition. Same to be renewed.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Inappropriate Procedure","10.38","Medium","","","Mating renewed after completion of cosmetic maintenance of the area.","2021-08-20","","Completed","2021-08-06","No","No","No","Internal"]
[null,null,null,null,20241,"54_31/07/2021 1:53:32 PM","2021-07-29","Defect,Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Port side davit limit switch to be renewed.","LSA / FFA","Emgcy. Systems","Equipment Related","5.29","High","","","Renewed with new spare onbaord.","2021-08-06","","Completed","2021-08-04","No","No","No","Internal"]
[null,null,null,null,20242,"54_31/07/2021 1:57:18 PM","2021-07-29","Other","Ship Staff","Suptd. Insp.","Various big valves at bottom platform needs to be painted as dry rust marks from docking time are still there.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.3","Medium","","","valves de-rusting , cleaning and painting carried out.","2021-08-10","","Completed","2021-08-05","No","No","No","Internal"]
[null,null,null,null,20243,"54_31/07/2021 2:01:39 PM","2021-07-29","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Both LT cooler has various rust weep marks. Same to be upgraded","E/R - Aux. Mach.,E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","After completion of Backflushing of both LT cooler, Cleaning and painting to be done. Marks wirebrushed and cleaned. Painted over","2021-08-20","","Completed","2021-08-31","No","No","No","Internal"]
[null,null,null,null,20244,"54_31/07/2021 2:04:49 PM","2021-07-29","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Sides near the DG platform to be cleaned.","Miscellaneous","Eng. / Strg. Comp.","External Factors","10.3","Medium","","","Cleaning to be done","2021-08-30","","Completed","2021-08-24","No","No","No","Internal"]
[null,null,null,null,20245,"54_31/07/2021 2:14:46 PM","2021-07-29","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Fire line outside purifier room to be painted","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.3","Medium","","","Old Paint Scrapped off and New paint applied","2021-08-07","","Completed","2021-08-06","No","No","No","Internal"]
[null,null,null,null,20246,"54_31/07/2021 2:17:06 PM","2021-07-29","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Bilges top to be cleaned and painted","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.3","Medium","","","Once bottom paintaing and cleaning completed. E/R tank to clean and painting to be done","2021-08-30","","Completed","2021-08-23","No","No","No","Internal"]
[null,null,null,null,20247,"54_31/07/2021 2:19:33 PM","2021-07-29","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","EGCS sea chest filter to be painted from top.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","De-rusted and painted from top..","2021-08-15","","Completed","2021-08-05","No","No","No","Internal"]
[null,null,null,null,20248,"54_31/07/2021 2:03:19 PM","2021-07-29","Defect,Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Leakage sighted near LO cooler port side. To be corrected and area to be cleaned.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Lekage to be identifed from Quick Closing valve of Aux DG. Gland tightened and cleaning carried out.","2021-08-10","","Completed","2021-08-06","No","No","No","Internal"]
[null,null,null,null,20249,"54_31/07/2021 2:21:22 PM","2021-07-29","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Steam leak near ME lubricator platform from tracing steam to be rectified.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Leaked traced, union tightned and leak rectified.","2021-08-20","","Completed","2021-08-05","No","No","No","Internal"]
[null,null,null,null,20250,"54_31/07/2021 2:23:43 PM","2021-07-29","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Neutralizing agent stored in EGCs room needs to be shifted near BWTS.","Miscellaneous","General Appearance","Equipment Related","11.2","Medium","","","Shifted to BWTS room.","2021-08-15","","Completed","2021-08-15","No","No","No","Internal","Target date revised."]
[null,null,null,null,20251,"54_31/07/2021 2:29:21 PM","2021-07-29","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Unit cooler outside ECR is not secured properly.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.3","Medium","","","Unit Cooler is secured in base nad tighteness checked","2021-08-07","","Completed","2021-08-06","No","No","No","Internal"]
[null,null,null,null,20252,"54_31/07/2021 03:10:59 AM","2021-07-29","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Pump room entrance door step is corroded from one side. To repair by bolting a plate on it.","Miscellaneous","Mooring","Equipment Related","11.3","Medium","","","Rectified and painted","2021-08-13","","Completed","2021-08-02","No","No","No","Internal"]
[null,null,null,null,20253,"54_31/07/2021 03:16:48 AM","2021-07-29","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Various shelters on deck to derust and paint","Miscellaneous","General Appearance","Equipment Related","11.3","Medium","","","Derusting and painting carried out","2021-08-29","","Completed","2021-08-28","No","No","No","Internal"]
[null,null,null,null,20254,"54_31/07/2021 03:22:28 AM","2021-07-29","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Both side manifold gratings to derust and paint.","Miscellaneous","General Appearance","External Factors","11.3","Medium","","","Derusting and painting of grating to be carried out .","2021-10-31","","Completed","2021-09-30","No","No","No","Internal","What is progress on it, How much % completed? Target date revised."]
[null,null,null,null,20255,"54_31/07/2021 03:25:34 AM","2021-07-29","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Both HHC platform grating to de-rust and paint.","Miscellaneous","General Appearance","External Factors","11.3","Medium","","","Derusting and painting completed ","2021-12-31","","Completed","2021-12-24","No","No","No","Internal","Understand job is in progress as weather permits. In consultation with TM the target date revised more than allowed limit."]
[null,null,null,null,20256,"54_31/07/2021 03:31:51 AM","2021-07-29","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","D deck port side entrance door latch is damaged, same to be replaced.","Accommodation","Structural Condn. / WT integrity ","Equipment Related","5.1","Very High","","","Vessel will replace the damaged door latch with new latch","2021-08-22","","Completed","2021-08-13","No","No","No","Internal"]
[null,null,null,null,20257,"54_31/07/2021 03:41:12 AM","2021-07-29","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Dry provision room, insulation mat near provision room panel is damaged, to be replaced.","Accommodation,Miscellaneous","Safety / LSA / FFA","Inappropriate Procedure","10.24","Low","","","Insualtion Mat replaced with new mat","2021-08-05","","Completed","2021-08-02","No","No","No","Internal"]
[null,null,null,null,20258,"54_31/07/2021 03:49:15 AM","2021-07-29","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Ballast pump foundation plate to derust and paint","Miscellaneous","Cargo / Ballast Systems","External Factors","11.3","Medium","","","Derusting and painting carried out on the foundation of ballast pumps","2021-08-09","","Completed","2021-08-02","No","No","No","Internal"]
[null,null,null,null,20259,"54_31/07/2021 03:54:41 AM","2021-07-29","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Most of the stanchion chains on deck are rusted.","Miscellaneous","General Appearance","External Factors","11.3","Medium","","","Stanchion chains derusted and painted ","2021-12-29","","Completed","2021-12-22","No","No","No","Internal","Understand job is in progress, Target date revised in consultation with TM more than the allowed limit."]
[null,null,null,null,20260,"54_31/07/2021 03:56:22 AM","2021-07-29","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Various panels in forepeak store needs to be cleared off dust on top of it.","Miscellaneous","General Appearance","External Factors","","","","","Fore peak store area including panel cleaned and squared up . ","2021-08-08","","Completed","2021-08-02","No","No","No","Internal"]
[null,null,null,null,20261,"54_31/07/2021 04:06:56 AM","2021-07-29","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","EGCS room various weathertight door does not have open – close marking. ","Miscellaneous","General Appearance","External Factors","11.3","Medium","","","derusting and painting to be carried out as weather permits","2021-08-13","","Completed","2021-08-10","No","No","No","Internal"]
[null,null,null,null,20262,"54_31/07/2021 03:46:39 AM","2021-07-29","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Fire control station foam tank rear side and used as store, many items are found stacked up there.  Same to be cleared and arranged.","Accommodation","Safety / LSA / FFA","Inappropriate Procedure","11.13","Low","","","Fire controal station area cleaned and squraed up . All unwanted items removed and stored in deck store","2021-08-06","","Completed","2021-08-06","No","No","No","Internal"]
[null,null,null,null,20263,"54_31/07/2021 04:08:37 AM","2021-07-29","Observation","Owner / Marine / Tech. Suptd.","Ship Staff Insp.","Port side LO bunkering manifold – LS Cyl oil bunkering pipe is badly rusted at bottom. To derust and paint and repair if require.","Miscellaneous","General Appearance","External Factors","","","","","Derusting and painting carried out","2021-08-22","","Completed","2021-08-20","No","No","No","Internal"]
[null,null,null,null,22226,"54_26/10/2021 09:57:22 AM","2021-08-06","Observation","Owner / Marine / Tech. Suptd.","Cargo Audit","22-June 2021 : Loading at Zikru Island:\n\nIn the ship-shore agreement, Initial loading rate was not specified, both ship & terminal rate were declared. There should be only one agreed/final rate.\n\n\n\n\n\n","Documentation","Cargo / Ballast Systems","Human Error","5.9","Very High","","","Checklist corrected. Master carried briefing session on correct filling of Ship shore agrrement","2021-11-05","","Completed","2021-09-02","No","No","No","Internal"]
[null,null,null,null,22227,"54_26/10/2021 10:01:43 AM","2021-08-06","Observation","Owner / Marine / Tech. Suptd.","Cargo Audit","22-June 2021 : Loading at Zikru Island:\n\nIn the ship-shore agreement, Topping off rate was not specified, both ship & terminal rate were declared. There should be only one agreed/final rate.\n\n","Documentation","Cargo / Ballast Systems","Human Error","5.9","Very High","","","Checklist corrected.Master briefed all officers on correct procedures for filling of checklist","2021-11-05","","Completed","2021-09-02","No","No","No","Internal"]
[null,null,null,null,22228,"54_26/10/2021 10:04:00 AM","2021-08-06","Observation","Owner / Marine / Tech. Suptd.","Cargo Audit","22-June 2021 : Loading at Zikru Island:\n\nIn the ship-shore agreement, Emergency stop procedure was left with “As per SSSCL” comments. ","Documentation","Cargo / Ballast Systems","Human Error","5.9","Very High","","","Checklist corrected.Master briefed all officers on correct procedures for filling of checklist","2021-11-05","","Completed","2021-09-02","No","No","No","Internal"]
[null,null,null,null,22229,"54_26/10/2021 10:05:57 AM","2021-08-06","Observation","Owner / Marine / Tech. Suptd.","Cargo Audit","22-June 2021 : Loading at Zikru Island:\n\nIn the ship-shore agreement, “Ship/shore stop” was left blank.\n\n","Documentation","Cargo / Ballast Systems","Human Error","5.9","Very High","","","Checklist corrected .Master briefed all officers on correct procedures for filling of checklist","2021-11-05","","Completed","2021-09-02","No","No","No","Internal"]
[null,null,null,null,22230,"54_26/10/2021 10:08:13 AM","2021-08-06","Observation","Owner / Marine / Tech. Suptd.","Cargo Audit","22-June 2021 : Loading at Zikru Island:\n\nThe ship-shore safety checklist was printed out without having checklist reference (I;e checklist no, name ,page no ) in it at the bottom.","Documentation","Cargo / Ballast Systems","Human Error","5.9","Very High","","","checklists corrected .Master briefed all officers on correct procedures for filling of checklist","2021-11-05","","Completed","2021-09-02","No","No","No","Internal"]
[null,null,null,null,22231,"54_26/10/2021 10:11:22 AM","2021-08-06","Observation","Owner / Marine / Tech. Suptd.","Cargo Audit","15-July 2021 : Discharging at Onsan,South Korea : \n\nPage no-11, item no 51 of ship shore checklist, “Emergency signal “left empty for tanker.\n\n","Documentation","Cargo / Ballast Systems","Human Error","5.9","Very High","","","Checklist corrected.Master briefed all officers on correct procedures for filling of checklist","2021-11-05","","Completed","2021-09-02","No","No","No","Internal"]
[null,null,null,null,21717,"54_22/10/2021 6:19:41 PM","2021-09-13","Observation","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","A review of the records indicated that ODME was used to disposed washing water from Slop P/S on 19 April 2021 and 21 April 2021 with the flow meter set to Manual Mode. An email communication with Flag state and relevant risk assessment prior using the ODME unit were presented by the Master. However the “Time of system failure”( Under code M) were not recorded in Oil Record Book Part II.","Cargo Mach.","MARPOL Related","Human Error","2.1","Very High","","","Training Carried to all crew on correct procedures for oil record book entries as per Intertanko guidelines ","2021-09-29","","Completed","2021-09-17","No","No","No","External"]
[null,null,null,null,24400,"54_18/03/2022 6:14:55 AM","2021-09-21","Observation","Ship Staff","Ship Staff Insp.","LT COOL P/P NO. 3 MOTOR GIVING SMELL AND ABNORMAL SOUND. ","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","MOTOR C/O AND DISMANTLED FOR O/H. FOUND BEARING SLACK IN HOUSING. SAME PUNCHED AND REFITTED WITH NEW BEARINGS AFTER CLEANING MOTOR AND RE- VARNISHING.","2021-09-24","","Completed","2021-09-21","No","No","No","Internal"]
[null,null,null,null,24401,"54_18/03/2022 6:03:30 AM","2021-09-24","Observation","Ship Staff","Ship Staff Insp.","AIRCON NO. 2 MOTOR MAKING ABNORMAL SOUND AND BURNING SMELL","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","MOTOR DISMANTLED FOR REPAIR ON 25TH SEP 2021. NEW MOTOR ORDERED . RECEIVED AND INSTALLED","2021-12-31","","Completed","2021-11-03","No","No","No","Internal"]
[null,null,null,null,21291,"54_30/09/2021 5:58:52 PM","2021-09-30","Defect","Ship Staff","Ship Staff Insp.","Sat C No 2 -Manual selection of Navarea is not possible ","Navigation - GMDSS & Communication","Communication","Equipment Related","4.21","High","","","Require Shore techinician assistance ","2021-12-31","","Completed","2021-10-28","No","No","No","Internal"]
[null,null,null,null,21292,"54_30/09/2021 6:02:44 PM","2021-09-30","Other","Ship Staff","Ship Staff Insp.","Stbd lifeboat has its sprinkler line holed and patched temporarily with soft patch ","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.28","Very High","","","Stbd Lifeboat Sprikler drain line was mis construed as drain line and hence closed ","2021-12-31","","Completed","2021-10-01","No","No","No","Internal","Share some pictures."]
[null,null,null,null,21293,"54_30/09/2021 6:06:33 PM","2021-09-30","Other","Ship Staff","Ship Staff Insp.","Approximately 10 nos of Intrinisically safe light foundation brackets in way of pumproom and accomodation decks found to wasted and holed","Elect. Mach. & Equip.","General Appearance","Equipment Related","11.9","Low","","","Wasted accomodation light base brackets attended ","2021-12-30","","Completed","2021-11-12","No","No","No","Internal"]
[null,null,null,null,24402,"54_18/03/2022 5:54:17 AM","2021-10-29","Defect","Ship Staff","Ship Staff Insp.","T/G VACUUM P/P MOTOR SHOWING LOW INSULATION","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","MOTOR DISMANTLED AND OVERHAUL. WINDING BREAK VISIBLE- SAME REPAIRED. BEARINGS RENEWED. NEW MOTOR ORDERED AS A PRECAUTION.DRED210231","2022-02-28","DRED210231","Completed","2021-12-08","No","No","No","Internal"]
[null,null,null,null,22528,"54_03/11/2021 1:58:11 PM","2021-11-02","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Empty wooden box from EGCS room to remove.","Miscellaneous","General Appearance","External Factors","","","","","Removed already.","2021-11-09","","Completed","2021-11-03","No","No","No","Internal"]
[null,null,null,null,22521,"54_02/11/2021 06:44:21 PM","2021-11-02","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Fiber gratings on deck are still secured with band-it strap. Use proper securing clamp and remove the band","Miscellaneous","General Appearance","Equipment Related","11.1","High","","","Vessel removed bands from all the gratings on deck . Replace bands with clamps for securing of gratings","2021-11-22","","Completed","2021-11-07","No","No","No","Internal"]
[null,null,null,null,22522,"54_02/11/2021 06:48:42 PM","2021-11-02","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Angle indicator of gangway in use ( Stbd Side) was missing.","Deck - Machinery","Safety / LSA / FFA","Equipment Related","5.47","Medium","","","Vessel will installed angle indicator on stbd gangway ","2021-11-09","","Completed","2021-11-07","No","No","No","Internal"]
[null,null,null,null,22523,"54_03/11/2021 1:51:19 PM","2021-11-02","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Stbd LT cooler SW pipe has leak marks. To tighten and clean.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Flange tightened and painted under observation. Flange tighetend and painted - no leaks.","2021-11-12","","Completed","2021-11-03","No","No","No","Internal"]
[null,null,null,null,22524,"54_03/11/2021 1:55:57 PM","2021-11-02","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","E/R entrance door from EGCS room, does not have open / close marking.","Miscellaneous","General Appearance","Human Error","","","","","Will be done shortly. Completed","2021-11-16","","Completed","2021-11-03","No","No","No","Internal"]
[null,null,null,null,22525,"54_03/11/2021 2:02:48 PM","2021-11-02","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Engine blower room ceiling to derust and paint.  Ceiling grating to secure.","Miscellaneous","General Appearance","External Factors","","","","","Cleaning and painting in progress. painting done","2021-12-02","","Completed","2021-11-06","No","No","No","Internal"]
[null,null,null,null,22526,"54_02/11/2021 06:46:32 PM","2021-11-02","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Elevator door lock at various deck are not in order. To renew.","Accommodation","General Appearance","Equipment Related","","","","","Vessel will inspect and renew doors handle locks as required. Door locks handle springs of E deck, B deck and Sunken deck found broken- same renewed from spares.","2021-12-02","","Completed","2021-11-03","No","No","No","Internal"]
[null,null,null,null,22527,"54_03/11/2021 2:00:41 PM","2021-11-02","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Emergency escape passage at E/R bottom platform to clean.","Miscellaneous","General Appearance","External Factors","","","","","Already cleaned and painted.","2021-11-09","","Completed","2021-11-02","No","No","No","Internal"]
[null,null,null,null,19843,"54_29/06/2021 12:57:49 AM","2021-11-04","Defect","Ship Staff","Ship Staff Insp.","EGB Soot Blower No.3 found Seized. Not roatating","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Motor found free and roatating, but lance seized.Complete Soot Blower along with lance to removed and easing to be carried out at next possible anchorage/Opportunity.Awaiting suitable opportunity.( Motor and lance removed) Awaiting pressure bearing supply. sootblower lance repaired on board and fitted in place.Ready for use.","2022-01-31","DRED210155","Completed","2022-01-12","No","No","No","Internal","Attend at next anchorage in load port"]
[null,null,null,null,24403,"54_17/03/2022 8:57:57 AM","2021-11-06","Observation","Ship Staff","Ship Staff Insp.","AE-2 LO ANALYSIS RETURNS CAUTION WITH HIGH CU CONTENT","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","OIL CHANGED, SUMP CLEANED, RANDOM BEARING INSPECTED. FRESH OIL TAKEN. NEW SAMPLE LANDED , RESULT NORMAL.","2021-12-15","","Completed","2021-12-06","No","No","No","Internal"]
[null,null,null,null,null,"54_17/03/2022 6:33:19 AM","2021-11-13","Other","Ship Staff","Ship Staff Insp.","Main Air Compressor No. 1 NR v/v leaking ","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related",null,null,"Not Applicable","Not Applicable","Beyond repair. ROB Nil. RO raised. Compressor isolated. Spare received and fitted.","2022-07-31","DRED 210240","Completed","2022-03-28","No",null,null,"Internal"]
[null,null,null,null,null,"54_18/03/2022 6:27:42 AM","2021-12-03","Observation","Ship Staff","Ship Staff Insp.","IG MAIN VALVE POSITIONER DEFECTIVE. NEW POSITIONER ORDERED VIDE DRED220002. SUPPLY AWAITED","Inert Gas","Eng. / Strg. Comp.","Equipment Related",null,null,"Not Applicable","Not Applicable","VALVE BEING OPERATED MANUALLY. POSITIONER SUPPLY AWAITED.positioner received and fitted in place. will be tried out at next opportunity","2022-06-30","DRED220002","Completed","2022-03-30","No",null,null,"Internal"]
[null,null,null,null,24155,"54_04/03/2022 9:44:56 AM","2021-12-08","Observation","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","The lubricating oil analysis report dated 5 Nov 2021 was noted with critical rating for Auxiliary Engine No. 2 that the oil was not suitable for further use provided the landed used oil sample was representative for the application. Elemental analysis show significant wear rate of Copper. Bearing might be the wear source of COPPER. Wear source of Copper shall be identified and appropriate corrective measures to be taken. Ship staff reported that the oil has been drained and the sump tank was cleaned. The Lubricating oil has been renewed and sample landed for analysis.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.7","Medium","","","Lube Oil Replinshed and landed at Singapore and Report found normal ","2022-12-31","","Completed","2021-12-15","No","No","No","External"]
[null,null,null,null,24404,"54_17/03/2022 8:49:30 AM","2021-12-14","Defect","Ship Staff","Ship Staff Insp.","HIGH LO CONSUMPTION AND BLOW PAST ","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","UNIT DISMANTLED AND DECARBONIZED. nEW PISTON RINGS, BIG END BEARING, PISTON ROD AND BEARI NG NUT AND BOLTS.OHAULED CYLINDER HEAD USED. ENGINE TRIED OUT AND RUN UP TO LOAD AS PER LOAD PROGRAM","2021-12-20","","Completed","2021-12-18","No","No","No","Internal"]
[null,null,null,null,24405,"54_17/03/2022 8:42:29 AM","2021-12-23","Defect","Ship Staff","Ship Staff Insp.","AE2 #4 UNIT EXHAUST TEMPERATURE HIGH, COMPRESSION AND PEAK PRESSURE LOW. ","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","UNIT DISMANTLED AND DECARBONIZED. nEW PISTON RINGS, BIG END BEARING, PISTON ROD AND BEARI NG NUT AND BOLTS.OHAULED CYLINDER HEAD USED. ENGINE TRIED OUT AND RUN UP TO LOAD AS PER LOAD PROGRAM","2021-12-31","","Completed","2021-12-26","No","No","No","Internal"]
[null,null,null,null,24406,"54_18/03/2022 5:38:20 AM","2022-01-07","Defect","Ship Staff","Ship Staff Insp.","MAC- SPERRE HMI PANEL BURNT","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related","","","","","MAKER INFORMED. SUPPLIED HMI PANEL UNDER WARRANTY. SAME FITTED AFTER CERTAIN QUERIES FOR CLARIFICATION REGARDING NEW UNIT.","2022-03-31","","Completed","2022-03-01","No","No","No","Internal"]
[null,null,null,null,null,"54_18/03/2022 11:11:43 AM","2022-01-08","Defect","Ship Staff","Ship Staff Insp.","VAPOUR MANIFOLD VALVE STBD SIDE AFT OPERATING WHEEL FREE TEETH OF GEAR WORN OUT AND VALVE IN CLOSED POSITION.VALVE TO BE RENEWED.\t","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related",null,null,"Not Applicable","Not Applicable","AWAITING SUPPLY OF VAPOUR VALVE REQUISITION RAISED DRED220004.SPARE RECEIVED AND FITTED IN PLACE. JOB COMPLETED.","2022-05-30","DRED220004","Completed","2022-03-29","No",null,null,"Internal"]
[null,null,null,null,23869,"54_15/02/2022 11:26:50 PM","2022-02-12","Defect","Ship Staff","Cargo Audit","During Pressure testing of steam coils of slop tank  1 no of steam trap found leaking","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.15","High","","","Steam trap Replaced ","2022-02-28","","Completed","2022-02-23","No","No","No","Internal","Is spare steam trap available onbaord?"]
[null,null,null,null,24154,"54_01/03/2022 09:18:22 AM","2022-02-26","Observation","Ship Staff","Ship Staff Insp.","Weather tight door Packing for Funner doors and Battery door room damaged and to be renewed.","Accommodation","Structural Condn. / WT integrity ","Equipment Related","10.44","Medium","","","Damaged Packings Replaced ","2022-03-30","","Completed","2022-03-06","No","No","No","Internal"]
[null,null,null,null,null,"54_18/03/2022 6:21:10 AM","2022-03-02","Defect","Ship Staff","Ship Staff Insp.","EGCS NO. 1 SEA WATER PUMP MOTOR BURNT.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related",null,null,"Not Applicable","Not Applicable","SYSTEM RUN WITH ONE PUMP. NEW MOTOR ORDERD VIDE DRED 220049.  NEW MOTOR RECEIVED ON 12/03/22 . IN CONVERSATION WITH MAKER REGARDING VFD ISSUES. MOTOR RECEIVED AT TIANJIN AND FITTED IN PLACE. VFD ISSUES SORTED OUT IN CONSULTATION WITH MAKER.","2022-03-31","DRED 220049","Completed","2022-03-19","No",null,null,"Internal"]
[null,null,null,null,24407,"54_18/03/2022 7:30:12 AM","2022-03-04","Observation","Ship Staff","Ship Staff Insp.","OWS FLOTATION TANK CRACKED ","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","SAME REPAIRED WITH COLD WORK. ANODES RENEWED.","2022-03-10","","Completed","2022-03-10","No","No","No","Internal"]
[null,null,null,null,24408,"54_17/03/2022 6:16:07 AM","2022-03-14","Observation","Ship Staff","Ship Staff Insp.","Slight leak from Riser line of No. 1 fuel pump of M/E","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Drain blown through and cleared with diesel. External leak stopped","2022-03-15","","Completed","2022-03-14","No","No","No","Internal"]

{"sheet":"Calc","index":2,"n_rows":28,"n_cols":12,"rows_kept":28,"cut":false,"hidden":true,"merged":[]}
["Def_type","Def_cause","Equipments","VIQrefno","Observer_code"]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,"Dim itemSele As Long"]
[null,null,null,null,null,null,null,null,null,null,null,"   dim startRow as integer"]
[null,null,null,null,null,null,null,null,null,null,null,"   startRow=1"]
[null,null,null,null,null,null,null,null,null,null,null,"        For itemSele = 0 To ListBox1.ListCount - 1"]
[null,null,null,null,null,null,null,null,null,null,null,"        If ListBox1.Selected(itemSele) = True Then"]
[null,null,null,null,null,null,null,null,null,null,null,"        Worksheets(\"WorksheetName\").Range(\"A\" & startRow).Value = ListBox1.List(itemSele)"]
[null,null,null,null,null,null,null,null,null,null,null,"        startRow = startRow + 1"]
[null,null,null,null,null,null,null,null,null,null,null,"        End If"]
[null,null,null,null,null,null,null,null,null,null,null,"        Next"]
[null,null,null,null,null,null,null,null,null,null,null,"Dim LastRowA As String"]
[null,null,null,null,null,null,null,null,null,null,null,"        Dim itemSele As Long"]
[null,null,null,null,null,null,null,null,null,null,null,"       Dim startRow as integer"]
[null,null,null,null,null,null,null,null,null,null,null,"        LastRowA = ActiveSheet.Cells(Rows.count, \"A\").End(xlUp).row"]
[null,null,null,null,null,null,null,null,null,null,null,"        startQue = 0"]
[null,null,null,null,null,null,null,null,null,null,null,"        For itemSele = 0 To ListBox1.ListCount - 1"]
[null,null,null,null,null,null,null,null,null,null,null,"        For startRow = 1 To LastRowA"]
[null,null,null,null,null,null,null,null,null,null,null,"        If Worksheets(\"WorksheetName\").Range(\"A\" & startRow).Value = ListBox1.List(itemSele) Then"]
[null,null,null,null,null,null,null,null,null,null,null,"        ListBox1.Selected(itemSele) = True"]
[null,null,null,null,null,null,null,null,null,null,null,"        Exit For"]
[null,null,null,null,null,null,null,null,null,null,null,"        End If"]
[null,null,null,null,null,null,null,null,null,null,null,"        Next j"]
[null,null,null,null,null,null,null,null,null,null,null,"        Next"]
[null,null,null,null,null,null,null,null,null,null,null,"        End If"]

{"sheet":"Areaofobs","index":3,"n_rows":17,"n_cols":2,"rows_kept":17,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Cargo / Ballast Systems",11]
["Cert. & Docu.",2]
["Communication",6]
["Crew Management",3]
["Emgcy. Systems",13]
["Eng. / Strg. Comp.",14]
["General Appearance",15]
["Ice Opns.",17]
["ISM Related",7]
["ISPS Related",10]
["MARPOL Related",9]
["MLC Related",4]
["Mooring",12]
["Navigation",5]
["Safety / LSA / FFA",8]
["Structural Condn. / WT integrity ",16]

{"sheet":"Vessel_type","index":4,"n_rows":1,"n_cols":2,"rows_kept":1,"cut":false,"hidden":true,"merged":[]}
["Vessel_type","ID"]

{"sheet":"Deficiency_type","index":5,"n_rows":8,"n_cols":3,"rows_kept":8,"cut":false,"hidden":true,"merged":[]}
["TITLE","Type of deficiency_description","ID"]
["Breakdown",null,6]
["Critical Equipment",null,4]
["Defect",null,1]
["Guarantee Claim",null,8]
["Non Conformity",null,2]
["Observation",null,3]
["Other",null,7]

{"sheet":"VIQrefno","index":6,"n_rows":427,"n_cols":3,"rows_kept":427,"cut":false,"hidden":true,"merged":[]}
["VIQ_ref_no","Risk Value of observation","ID"]
["1.1","Low",8243]
["1.10","Low",8252]
["1.11","Low",8253]
["1.12","Low",8254]
["1.13","Low",8255]
["1.14","Low",8256]
["1.15","Low",8257]
["1.16","Low",8259]
["1.17","Low",8260]
["1.18","Low",8261]
["1.19","Low",8262]
["1.2","Low",8244]
["1.20","Low",8263]
["1.21","Low",8265]
["1.22","Low",8266]
["1.23","Low",8267]
["1.24","Low",8268]
["1.25","Low",8269]
["1.26","Low",8270]
["1.3","Low",8245]
["1.4","Low",8246]
["1.5","Low",8247]
["1.6","Low",8248]
["1.7","Low",8249]
["1.8","Low",8250]
["1.9","Low",8251]
["1.99","High",11258]
["10.1","Medium",8461]
["10.10","High",8470]
["10.11","Medium",8471]
["10.12","Very High",8472]
["10.13","Very High",8473]
["10.14","Medium",8474]
["10.15","Low",8475]
["10.16","Very High",8476]
["10.17","Very High",8477]
["10.18","High",8478]
["10.19","Very High",8479]
["10.2","Low",8462]
["10.20","High",8480]
["10.21","Medium",8481]
["10.22","Low",8482]
["10.23","Medium",8483]
["10.24","Low",8484]
["10.25","Very High",8485]
["10.26","High",8486]
["10.27","Medium",8487]
["10.28","Low",8488]
["10.29","Medium",8489]
["10.3","Medium",8463]
["10.30","High",8490]
["10.31","Very High",8491]
["10.32","Very High",8492]
["10.33","High",8493]
["10.34","High",8494]
["10.35","Very High",8495]
["10.36","Very High",8496]
["10.37","Medium",8497]
["10.38","Medium",8498]
["10.39","High",8499]
["10.4","High",8464]
["10.40","Medium",8500]
["10.41","Medium",8501]
["10.42","Medium",8502]
["10.43","Medium",8503]
["10.44","Medium",8504]
["10.45","Very High",8505]
["10.46","High",8506]
["10.47","Medium",8507]
["10.48","High",8508]
["10.49","Medium",8509]
["10.5","Low",8465]
["10.50","High",8510]
["10.51","Low",8511]
["10.52","Medium",8512]
["10.53","Medium",8513]
["10.54","High",8514]
["10.55","Low",8515]
["10.6","Very High",8466]
["10.7","Medium",8467]
["10.8","Medium",8468]
["10.9","Medium",8469]
["10.99","High",8516]
["11.1","High",8420]
["11.10","Medium",8429]
["11.11","Very High",8430]
["11.12","Low",8431]
["11.13","Low",8432]
["11.14","Medium",8433]
["11.15","Low",8434]
["11.16","Low",8435]
["11.17","Low",8436]
["11.2","Medium",8421]
["11.3","Medium",8422]
["11.4","Very High",8423]
["11.5","Medium",8424]
["11.6","Medium",8425]
["11.7","High",8426]
["11.8","Low",8427]
["11.9","Low",8428]
["11.99","High",8437]
["12.1","High",8438]
["12.10","High",8448]
["12.11","High",8449]
["12.12","High",8450]
["12.13","High",8451]
["12.14","High",8452]
["12.15","High",8453]
["12.16","High",8454]
["12.17","High",8455]
["12.18","High",8456]
["12.19","High",8457]
["12.2","High",8439]
["12.20","High",8458]
["12.21","High",8459]
["12.3","High",8441]
["12.4","High",8442]
["12.5","High",8443]
["12.6","High",8444]
["12.7","High",8445]
["12.8","High",8446]
["12.9","High",8447]
["12.99","High",8460]
["2.1","Very High",8296]
["2.1.9","Very High",11259]
["2.10","Medium",8304]
["2.11","Medium",8305]
["2.12","Low",8306]
["2.13","Low",8307]
["2.14","Low",8308]
["2.15","Low",8309]
["2.16","Medium",8310]
["2.2","Medium",8297]
["2.3","High",8295]
["2.4","Medium",8298]
["2.5","Medium",8299]
["2.6","Low",8300]
["2.7","High",8301]
["2.8","High",8302]
["2.9","Medium",8303]
["2.99","High",8311]
["3.1","High",8312]
["3.2","Very High",8313]
["3.3","High",8314]
["3.4","Low",8294]
["3.5","Medium",8315]
["3.6","High",8316]
["3.7","Very High",8317]
["3.8","Very High",8318]
["3.99","High",8319]
["4.1","High",8320]
["4.10","High",8329]
["4.11","Medium",8330]
["4.12","Very High",8331]
["4.13","Very High",8332]
["4.14","Very High",8333]
["4.15","Very High",8334]
["4.16","Very High",8335]
["4.17","Very High",8336]
["4.18","Very High",8337]
["4.19","Low",8338]
["4.2","Medium",8321]
["4.20","Very High",8339]
["4.21","High",8340]
["4.22","Low",8341]
["4.23","High",8342]
["4.24","High",8343]
["4.25","Low",8344]
["4.26","Low",8345]
["4.27","High",8346]
["4.3","Medium",8322]
["4.4","High",8323]
["4.5","Very High",8324]
["4.6","Medium",8325]
["4.7","High",8326]
["4.8","Medium",8327]
["4.9","Medium",8328]
["4.99","High",8347]
["5.1","Very High",8517]
["5.10","High",8526]
["5.11","Low",8527]
["5.12","Medium",8528]
["5.13","High",8529]
["5.14","Very High",8530]
["5.15","Medium",8531]
["5.16","Very High",8532]
["5.17","Very High",8533]
["5.18","High",8534]
["5.19","Medium",8535]
["5.2","Very High",8518]
["5.20","Medium",8536]
["5.21","Medium",8537]
["5.22","High",8539]
["5.23","Very High",8540]
["5.24","Very High",8541]
["5.25","Medium",8542]
["5.26","Medium",8543]
["5.27","Medium",8544]
["5.28","Very High",8545]
["5.29","High",8546]
["5.3","Low",8519]
["5.30","High",8547]
["5.31","High",8548]
["5.32","High",8549]
["5.33","High",8550]
["5.34","Low",8551]
["5.35","Medium",8552]
["5.36","Low",8553]
["5.37","Low",8554]
["5.38","High",8555]
["5.39","Very High",8556]
["5.4","High",8520]
["5.40","Very High",8557]
["5.41","Very High",8558]
["5.42","Medium",8559]
["5.43","High",8560]
["5.44","High",8561]
["5.45","Medium",8564]
["5.46","Medium",8565]
["5.47","Medium",8566]
["5.48","Medium",8567]
["5.5","Low",8521]
["5.6","Low",8522]
["5.7","Medium",8523]
["5.8","Medium",8524]
["5.9","Very High",8525]
["5.99","High",8568]
["6.1","Medium",8348]
["6.10","Low",8357]
["6.11","High",8358]
["6.12","Medium",8359]
["6.13","Low",8360]
["6.14","High",8361]
["6.15","High",8362]
["6.16","Very High",8363]
["6.17","Very High",8364]
["6.18","Medium",8365]
["6.19","Low",8366]
["6.2","High",8349]
["6.20","Medium",8367]
["6.21","High",8368]
["6.22","Medium",8369]
["6.3","Low",8350]
["6.4","High",8351]
["6.5","Medium",8352]
["6.6","Medium",8353]
["6.7","High",8354]
["6.8","High",8355]
["6.9","Low",8356]
["6.99","High",8370]
["7.1","High",8371]
["7.10","High",8380]
["7.11","High",8381]
["7.12","High",8382]
["7.13","Medium",8383]
["7.14","Medium",8384]
["7.15","High",8385]
["7.16","High",8386]
["7.17","High",8387]
["7.2","High",8372]
["7.3","Low",8373]
["7.4","Low",8374]
["7.5","Low",8375]
["7.6","Medium",8376]
["7.7","Low",8377]
["7.8","High",8378]
["7.9","High",8379]
["7.99","High",8388]
["8.1","Very High",8569]
["8.10","Very High",8578]
["8.100","Low",11227]
["8.101","Medium",11228]
["8.102","Low",11229]
["8.103","Low",11230]
["8.104","Low",11231]
["8.105","Medium",11232]
["8.106","Medium",11233]
["8.107","Low",11234]
["8.108","High",11235]
["8.109","Very High",11236]
["8.11","Medium",8579]
["8.110","High",11237]
["8.111","Medium",11238]
["8.112","High",11239]
["8.113","Medium",11240]
["8.114","Low",11241]
["8.115","High",11242]
["8.116","Medium",11243]
["8.117","Medium",11244]
["8.118","Medium",11245]
["8.119","High",11246]
["8.12","Medium",8580]
["8.120","High",11247]
["8.121","Medium",11248]
["8.122","High",11249]
["8.123","High",11250]
["8.124","Low",11251]
["8.125","High",11252]
["8.126","Medium",11253]
["8.127","Medium",11254]
["8.13","Medium",8581]
["8.14","Very High",8582]
["8.15","High",8583]
["8.16","Very High",8584]
["8.17","Low",8585]
["8.18","High",8586]
["8.19","High",8587]
["8.199","High",11255]
["8.2","Medium",8570]
["8.20","Medium",8588]
["8.21","High",8589]
["8.22","Very High",8590]
["8.23","Medium",8591]
["8.24","Medium",8592]
["8.25","Very High",8593]
["8.26","High",8594]
["8.27","Medium",8595]
["8.28","Medium",8596]
["8.29","High",8598]
["8.3","Very High",8571]
["8.30","High",8599]
["8.31","High",8600]
["8.32","Low",8601]
["8.33","Medium",8602]
["8.34","High",8603]
["8.35","Medium",8604]
["8.36","Medium",8605]
["8.37","High",8607]
["8.38","Medium",8608]
["8.39","Medium",8609]
["8.4","Medium",8572]
["8.40","High",8610]
["8.41","Medium",8611]
["8.42","Medium",8612]
["8.43","Very High",8613]
["8.44","High",8615]
["8.45","High",8616]
["8.46","Very High",8617]
["8.47","Very High",8618]
["8.48","Medium",8619]
["8.49","High",8620]
["8.5","Very High",8573]
["8.50","Medium",8621]
["8.51","Low",8622]
["8.52","Low",8623]
["8.53","Low",8624]
["8.54","High",8625]
["8.55","Low",11182]
["8.56","Medium",11183]
["8.57","Medium",11184]
["8.58","High",11185]
["8.59","High",11186]
["8.6","Medium",8574]
["8.60","High",11187]
["8.61","Medium",11188]
["8.62","Very High",11189]
["8.63","High",11190]
["8.64","Medium",11191]
["8.65","Low",11192]
["8.66","High",11193]
["8.67","High",11194]
["8.68","High",11195]
["8.69","Medium",11196]
["8.7","High",8575]
["8.70","Medium",11197]
["8.71","Very High",11198]
["8.72","Medium",11199]
["8.73","Medium",11200]
["8.74","High",11201]
["8.75","Medium",11202]
["8.76","Medium",11203]
["8.77","Medium",11204]
["8.78","Medium",11205]
["8.79","Medium",11206]
["8.8","Medium",8576]
["8.80","Medium",11207]
["8.81","Low",11208]
["8.82","Medium",11209]
["8.83","Low",11210]
["8.84","Low",11211]
["8.85","Medium",11212]
["8.86","Medium",11213]
["8.87","Medium",11214]
["8.88","Low",11215]
["8.89","High",11216]
["8.9","High",8577]
["8.90","High",11217]
["8.91","High",11218]
["8.92","Medium",11219]
["8.93","Low",11220]
["8.94","Low",11221]
["8.95","Medium",11222]
["8.96","Medium",11223]
["8.97","Low",11224]
["8.98","High",11225]
["8.99","Medium",11226]
["9.1","Low",8390]
["9.10","Medium",8399]
["9.11","Medium",8400]
["9.12","Medium",8401]
["9.13","Low",8402]
["9.14","Medium",8403]
["9.15","Medium",8404]
["9.16","High",8405]
["9.17","High",8406]
["9.18","Low",8407]
["9.19","Low",8408]
["9.2","Very High",8391]
["9.20","Medium",8409]
["9.21","Medium",8410]
["9.22","Low",8411]
["9.23","Low",8412]
["9.24","Medium",8413]
["9.25","Low",8414]
["9.26","Low",8415]
["9.27","Low",8416]
["9.28","Medium",8417]
["9.29","Low",8418]
["9.3","Very High",8392]
["9.4","High",8393]
["9.5","High",8394]
["9.6","Low",8395]
["9.7","Medium",8396]
["9.8","Medium",8397]
["9.9","Medium",8398]
["9.99","High",8419]

{"sheet":"Equipment_list","index":7,"n_rows":28,"n_cols":3,"rows_kept":28,"cut":false,"hidden":true,"merged":[]}
["TITLE","Equipment_list_description","ID"]
["Accommodation",null,12]
["Cargo Mach.",null,13]
["Critical Equip.",null,16]
["Deck - Machinery",null,18]
["Deck - Mooring Machinery",null,15]
["Deck - Pipe / Fittings",null,20]
["Documentation",null,21]
["E/R - Air Comp.",null,8]
["E/R - Aux. Engine",null,4]
["E/R - Aux. Mach.",null,7]
["E/R - Boiler",null,5]
["E/R - Main Engine",null,3]
["E/R - Pipes/ valves & fittings",null,9]
["E/R - Pumps",null,32]
["E/R - Purifier",null,6]
["Elect. Mach. & Equip.",null,10]
["Hull & Tanks",null,19]
["Inert Gas",null,14]
["LSA / FFA",null,17]
["Miscellaneous",null,22]
["Navigation - DGPS / EPFS / AIS",null,28]
["Navigation - ECDIS",null,25]
["Navigation - Echo Sounder / Speed Log",null,26]
["Navigation - GMDSS & Communication",null,23]
["Navigation - Others",null,11]
["Navigation - RADAR",null,24]
["Navigation - VDR / BNWAS",null,30]

{"sheet":"PSC_MOU","index":8,"n_rows":11,"n_cols":3,"rows_kept":11,"cut":false,"hidden":true,"merged":[]}
["TITLE","PSC_MOU_description","ID"]
["Asia and the Pacific",null,2]
["Caribbean",null,4]
["Europe and the North Atlantic",null,1]
["Latin America",null,3]
["The Black Sea region",null,6]
["The Indian Ocean",null,8]
["The Mediterranean",null,7]
["The Riyadh MoU",null,9]
["USCG",null,10]
["West and Central Africa",null,5]

{"sheet":"Inspection_type","index":9,"n_rows":13,"n_cols":2,"rows_kept":13,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Bunkering Audit",14]
["Cargo Audit",17]
["Engineering Audit",16]
["ISM Audit",2]
["ISPS Audit",3]
["IT Audit",10]
["MLC Audit",1]
["Mooring Audit",9]
["Nav Audit / Verification",8]
["Onboard Training",18]
["Ship Staff Insp.",15]
["Suptd. Insp.",13]

{"sheet":"Deficiency_Cause","index":10,"n_rows":8,"n_cols":3,"rows_kept":8,"cut":false,"hidden":true,"merged":[]}
["TITLE","Deficiency_Cause_description","ID"]
["Behaviour Based",null,1]
["Equipment Related",null,4]
["External Factors",null,5]
["Human Error",null,7]
["Inappropriate Procedure",null,8]
["Industry Issue",null,6]
["Knowledge Based",null,3]

{"sheet":"Observer_code","index":11,"n_rows":3,"n_cols":3,"rows_kept":3,"cut":false,"hidden":true,"merged":[]}
["TITLE","Observer_code_description","ID"]
["Owner / Marine / Tech. Suptd.",null,3]
["Ship Staff",null,2]

{"sheet":"Status_code","index":12,"n_rows":6,"n_cols":3,"rows_kept":6,"cut":false,"hidden":true,"merged":[]}
["TITLE","Status_code_description","ID"]
["Completed",null,6]
["Deferred to D D",null,5]
["In progress",null,3]
["Not Started",null,2]
["Waiting spare",null,4]

{"sheet":"PSC_ref_no","index":13,"n_rows":19,"n_cols":2,"rows_kept":19,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Alarms",9]
["Cargo operations including equipment",7]
["Certificates & Documentation",2]
["Dangerous Goods",13]
["Emergency Systems",5]
["Fire safety",8]
["ISM",16]
["ISPS",17]
["Life saving appliances",12]
["MLC, 2006",18]
["Other",19]
["Pollution Prevention",15]
["Propulsion and auxiliary machinery",14]
["Radio communication",6]
["Safety of Navigation",11]
["Structural condition",3]
["Water/Weathertight condition",4]
["Working and Living Conditions",10]

{"sheet":"Risk_value_of_obs","index":14,"n_rows":1,"n_cols":2,"rows_kept":1,"cut":false,"hidden":true,"merged":[]}
["Risk Value of observation","ID"]

{"sheet":"Year","index":15,"n_rows":18,"n_cols":1,"rows_kept":18,"cut":false,"hidden":true,"merged":[]}
["Year"]
[2014]
[2015]
[2016]
[2017]
[2018]
[2019]
[2020]
[2021]
[2022]
[2023]
[2024]
[2025]
[2026]
[2027]
[2028]
[2029]
[2030]

{"sheet":"Month","index":16,"n_rows":13,"n_cols":1,"rows_kept":13,"cut":false,"hidden":true,"merged":[]}
["Month"]
["Jan"]
["Feb"]
["Mar"]
["Apr"]
["May"]
["Jun"]
["Jul"]
["Aug"]
["Sep"]
["Oct"]
["Nov"]
["Dec"]

{"sheet":"Date_","index":17,"n_rows":32,"n_cols":1,"rows_kept":32,"cut":false,"hidden":true,"merged":[]}
["Date"]
["01"]
["02"]
["03"]
["04"]
["05"]
["06"]
["07"]
["08"]
["09"]
[10]
[11]
[12]
[13]
[14]
[15]
[16]
[17]
[18]
[19]
[20]
[21]
[22]
[23]
[24]
[25]
[26]
[27]
[28]
[29]
[30]
[31]

{"sheet":"Sheet1","index":18,"n_rows":24,"n_cols":6,"rows_kept":24,"cut":false,"hidden":true,"merged":[]}
[]
[null,"ID","E",null,"Date Recorded",1]
[null,"UNIQUE ID","F",null,"Type of Deficiency",2]
[1,"Date Recorded","G",null,"Observer code",3]
["ignore","Vessel Type","H",null,"Type of Inspection",4]
[null,"Internal / External","I",null,"Description of Deficiency",5]
[null,"Drydock","J",null,"Equipment Categories",6]
[null,"Information Sharing","K",null,"Area of Observation",7]
[null,"Critical_item","L",null,"Deficiency Cause",8]
[null,"Deficiency Type","M",null,"VIQ Ref Number",9]
[null,"Deficiency Cause","N",null,"Risk Value of Obs",10]
[null,"Inspection Type","O",null,"PSC Ref Number",11]
[null,"Equipments","P",null,"PSC MOU ID",12]
[null,"VIQ Reference Number","Q",null,"Action Taken or Required",13]
[null,"Risk Value of the observation","R",null,"Target Date",14]
[null,"PSC Reference Number","S",null,"PO Ref No.",15]
[null,"PSC MOU","T",null,"Status Code",16]
[null,"Observer Code","U",null,"Date Completed",17]
[null,"Target Date","V",null,"Drydock",18]
[null,"Status Code","W",null,"Info Sharing",19]
[null,"Description of Deficiency","X",null,"Critical Item Flag",20]
[null,"Action taken / required","Y",null,"Audit Type",21]
[null,"PO ref no","Z"]
[null,"Date completed","AA"]

{"sheet":"Ship_information","index":19,"n_rows":2,"n_cols":3,"rows_kept":2,"cut":false,"hidden":true,"merged":[]}
["Ship_ID","Ship_Name","FILE_NAME"]
["54","DHT REDWOOD (04-03-2022)","54_1647825082212.xlsm"]

{"sheet":"External_Deficiency_type","index":20,"n_rows":5,"n_cols":3,"rows_kept":5,"cut":false,"hidden":true,"merged":[]}
["TITLE","Type of deficiency_description","ID"]
["Condn of Class / Memo",null,5]
["Defect",null,1]
["Non Conformity",null,2]
["Observation",null,3]

{"sheet":"External_Inspection_type","index":21,"n_rows":11,"n_cols":2,"rows_kept":11,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Cargo Audit",17]
["Flag State Insp.",5]
["ISM Audit",2]
["ISPS Audit",3]
["MLC Audit",1]
["Nav Audit / Verification",8]
["OM Insp. (Eg. SIRE / CDI etc.)",6]
["Others (Eg. Insurance etc.)",12]
["PSC Inspection",4]
["Terminal Insp.",11]

{"sheet":"External_Observer_code","index":22,"n_rows":7,"n_cols":3,"rows_kept":7,"cut":false,"hidden":true,"merged":[]}
["TITLE","Observer_code_description","ID"]
["Class Surveyor",null,4]
["FSC Inspector",null,5]
["Others (Eg. Insurance etc.)",null,9]
["PSC Insp.",null,6]
["SIRE / CDI Insp.",null,8]
["Terminal Insp.",null,7]

{"sheet":"Sheet Version","index":23,"n_rows":2,"n_cols":2,"rows_kept":2,"cut":false,"hidden":true,"merged":[]}
["Version","Title"]
["2.0","Version 2.0"]