{"text_format":"1","workbook":"xlsx","n_sheets":24,"sheets":["Mainsheet","Completed","Calc","Areaofobs","Vessel_type","Deficiency_type","VIQrefno","Equipment_list","PSC_MOU","Inspection_type","Deficiency_Cause","Observer_code","Status_code","PSC_ref_no","Risk_value_of_obs","Year","Month","Date_","Sheet1","Ship_information","External_Deficiency_type","External_Inspection_type","External_Observer_code","Sheet Version"],"not_rendered":{"charts":0,"images":1,"macros":1,"external_links":0,"defined_names":12,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Mainsheet","index":0,"n_rows":34,"n_cols":28,"rows_kept":34,"cut":false,"hidden":false,"merged":[[10,8,10,9],[10,12,10,13],[12,6,12,27],[8,6,8,27]]}
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,"Defect - Damage Monitoring Sheet"]
[]
[null,null,null,null,null,null,null,"Date of Report","01-May-2022",null,null,"Ship Name","DHT SCANDINAVIA (22-04-2022)"]
[]
[null,null,null,null,null,null,"VERSION : 2.0"]
[]
[]
[]
[null,null,null,"ID","SHIPSIDE UNIQUEID","UNIQUE ID","Date Recorded","Type of Deficiency","Observer code","Type of Inspection","Description of Deficiency","Equipment Categories","Area of Observation","Deficiency Cause","VIQ Ref Number","Risk Value of Obs","PSC Ref Number","PSC MOU ID","Action Taken or Required","Target Date","PO Ref No.","Status Code","Date Completed","Drydock","Info Sharing","Critical Item","Audit Type","Superintendent Remarks"]
[null,null,null,20222,null,"45_31/07/2021 3:36:05 PM","2021-09-30T23:59:35","Observation","Ship Staff","Ship Staff Insp.","AE flow meter not working properly. Fuel oil consumtion and flow meter readings are irrelavent most of the times..","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Flow meter inspected, magnetic efect of the counter is not proper, due to that it is showing wrong counter reading . Required to renew the flow meter.New Flowmeter fitted but found still giving wrong readings.To be taken up with maker.Suspect bypass valve leaking.To be taken up at suitable anchorage to blank off the bypass valve.and observe","2022-05-31T23:59:35","scan210126","In progress",null,"No","No","No","Internal","on Order. Will be supplied once ready. Target date revised accordingly."]
[null,null,null,23169,null,"45_20/12/2021 1:48:45 PM","2021-12-19T23:59:35","Defect","Ship Staff","Ship Staff Insp.","A/E Auto back wash filter change over valve not holding","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","O' rings need to be replaced,filter cleaned by stopping the G/E F.O pumps and running the air operated F.O p/p.","2022-05-31T23:59:35","scan220067","Waiting spare",null,"No","No","No","Internal"]
[null,null,null,23780,null,"45_01/02/2022 11:17:58 AM","2022-01-09T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Oil mist detector for engine room found to be in setting mode","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","4 in number detector heads found defective, one new sensor replaced, PO raised for other 3 and 2 cooling fans changed from onboard available spare","2022-05-31T23:59:35","SCAN220020","Waiting spare",null,"No","No","No","Internal","Spares on order and will be connected once ready."]
[null,null,null,23541,null,"45_15/01/2022 3:11:08 PM","2022-01-09T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Sacrificial flange of port LT cooler leaking","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Sacrificial flange to be renewed, PO raised.Spare received.Shall combine with another defect WO(Pressuretapping  at LTcooler)","2022-05-31T23:59:35","SCAN220016","In progress",null,"No","No","No","Internal","Flange will be supplied in Singapore."]
[null,null,null,23546,null,"45_15/01/2022 4:04:40 PM","2022-01-09T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Port LT cooler pressure gauge tapping plugged","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Distance piece to be renewed .PO raised.","2022-05-31T23:59:35","SCAN220019","Waiting spare",null,"No","No","No","Internal"]
[null,null,null,23863,null,"45_15/02/2022 8:30:18 AM","2022-02-09T23:59:35","Observation","Ship Staff","Ship Staff Insp.","SOx value not increasing for the EGCS system","E/R - Main Engine,Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Discussion with maker in progress","2022-05-31T23:59:35","","In progress",null,"No","No","No","Internal"]
[null,null,null,24146,null,"45_21/02/2022 9:54:50","2022-02-17T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Gear for the Slop P (IG35) IG branch valve actuator was found damaged, actuator inoperational. Need to repalce the actuator.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.2","Medium","","","Presently operation of valve is by removing the actuator and turning the valve spindle using pipe wrench. RO raised - SCAN220053","2022-05-16T23:59:35","SCAN220053","Waiting spare",null,"No","No","No","Internal","Will be arranged supply."]
[null,null,null,24319,null,"45_07/03/2022 14:41:11","2022-03-03T08:00:00","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","VRCS junction box on deck near mid ship area requires to be de-rusted","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.8","Low","","","Repairing of the VRCS boxes in progress as the sides were wasted due to corrosion. Removed them to ER work shop for repairing","2022-05-03T08:00:00","","In progress",null,"No","No","No","Internal"]
[null,null,null,24944,null,"45_01/04/2022 12:44:23 PM","2022-03-28T23:59:35","Defect","Ship Staff","Ship Staff Insp.","NO.3 boiler feed water p/p aft side seal is having minor leak.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","spare mechanical sea onboard job planned after discharging.","2022-04-30T23:59:35","","Not Started",null,"No","No","No","Internal"]
[null,null,null,24945,null,"45_12/04/2022 15:32:33","2022-04-12T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Mast riser hydraulic valve- leaking from actuator due to worn out seal ring of the piston","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.11","Medium","","","Renew the worn out seal ring of the piston","2022-07-12T23:59:35","SCAN220098","Waiting spare",null,"No","No","No","Internal"]
[null,null,null,24946,null,"45_12/04/2022 15:37:15","2022-04-12T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Lifeboats fwd & aft securing gripe wires eyes are not mechanically spliced type as per maker manual.","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.29","High","","","Replace the existing ones with original type rope","2022-07-12T23:59:35","SCAN220095","Waiting spare",null,"No","No","No","Internal"]
[null,null,null,24947,null,"45_12/04/2022 15:40:24","2022-04-12T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Stripping pump discharge pressure transmitter faulty & requires replacement","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.8","Medium","","","Replace the faulty transmitter","2022-07-12T23:59:35","SCAN220092","Waiting spare",null,"No","No","No","Internal"]
[null,null,null,24948,null,"45_12/04/2022 16:01:46","2022-04-12T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Tank overfill alarm on bridge front- Strobe light body broken from the securing screws","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.14","Very High","","","Replace the light","2022-07-12T23:59:35","SCAN220097","Waiting spare",null,"No","No","No","Internal"]
[null,null,null,null,60570,"45_Mon Apr 25 2022 22:05:07 GMT+0800","2022-04-25T08:00:00","Observation","Ship Staff","Ship Staff Insp.","Cargo educator suction press & discharge gauge showing wrong reading in CCR.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.8","Medium","","","calibration carried out. Checked as per maker manual.\nRequire spare to renew the faulty gauge","2022-07-24T08:00:00","DHAW220092","Waiting spare",null,"No","No","No","Internal"]
[null,null,null,null,50096,"45_Mon Apr 25 2022 22:09:38 GMT+0800","2022-04-25T08:00:00","Observation","Ship Staff","Ship Staff Insp.","4S WBT main valve indicator transmitter in solenoid box is faulty.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.8","Medium","","","Require spare to replace the faulty one","2022-07-24T08:00:00","DHAW220107","Waiting spare",null,"No","No","No","Internal"]
[null,null,null,null,53707,"45_Mon Apr 25 2022 22:24:26 GMT+0800","2022-04-25T08:00:00","Observation","Ship Staff","Ship Staff Insp.","Magnetic compass of Port Side Lifeboat showing defectives readings.","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.29","High","","","Requisition (SCAN220095) for new Lifeboat Magnetic compass raised in PAL Awaiting spares.","2022-07-24T08:00:00","","Waiting spare",null,"No","No","No","Internal"]
[null,null,null,null,12124,"0_Mon Apr 25 2022 22:29:19 GMT+0800","2022-04-25T08:00:00","Observation","Ship Staff","Ship Staff Insp.","Foam Monitor no. 1 and 6 Valve leaking, Requires renewal of Valve since complete seat ring has been damaged.","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.35","Medium","","","Requisition (SCAN220095) raised in PAL vessel awaiting Sapres","2022-07-24T08:00:00","","Waiting spare",null,"No","No","No","Internal"]

{"sheet":"Completed","index":1,"n_rows":550,"n_cols":28,"rows_kept":550,"cut":false,"hidden":false,"merged":[[10,8,10,9],[10,12,10,13],[12,6,12,27],[8,6,8,27]]}
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,"Defect - Damage Monitoring Sheet"]
[]
[null,null,null,null,null,null,null,"Date of Report","01-May-2022",null,null,"Ship Name","DHT SCANDINAVIA (22-04-2022)"]
[]
[null,null,null,null,null,null,"VERSION : 2.0"]
[]
[]
[]
[null,null,null,"ID","SHIPSIDE UNIQUEID","UNIQUE ID","Date Recorded","Type of Deficiency","Observer code","Type of Inspection","Description of Deficiency","Equipment Categories","Area of Observation","Deficiency Cause","VIQ Ref Number","Risk Value of Obs","PSC Ref Number","PSC MOU ID","Action Taken or Required","Target Date","PO Ref No.","Status Code","Date Completed","Drydock","Info Sharing","Critical Item","Audit Type","Superintendent Remarks"]
[null,null,null,180,null,"45_Mon Oct 07 2019 02:34:48 GMT+0000","2019-01-06T23:59:35","Defect","Ship Staff","Ship Staff Insp.","DG LO purifier motor found with abnormal sound while running","E/R - Purifier","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Motor overhauled , bearings renewed,working satisfactory.JOB ORDER NO : (V-SCAN017100/19)","2019-01-07T23:59:35","","Completed","2019-01-07T23:59:35","No","No","No","Internal"]
[null,null,null,181,null,"45_Sat Oct 05 2019 23:29:13 GMT+0000","2019-01-07T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Window wiper ( No.2 Stbd side)  found not working ","Navigation - Others","Navigation","Equipment Related","12.1","High","","","Carriage plate renewed with new spare, working satifactory.JOB ORDER NO : (V-SCAN017039/19) ","2019-01-09T23:59:35","","Completed","2019-01-09T23:59:35","No","No","No","Internal"]
[null,null,null,182,null,"45_Mon Oct 07 2019 02:41:53 GMT+0000","2019-01-09T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Main air compressor#2 auto unloading valve found not operating ","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Renewed with spare valve, working satisfactory .JOB ORDER NO :(V-SCAN 017040/19)","2019-01-10T23:59:35","","Completed","2019-01-10T23:59:35","No","No","No","Internal"]
[null,null,null,194,null,"45_Mon Oct 07 2019 02:49:00 GMT+0000","2019-01-22T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Main engine fuel oil pressure transmitter found malfunctioning ( showing IFL & fluctuating frequently)","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Pressure transmitter renewed with new spare ,wiring checked, found working satisfactory.JOB ORDER NO :(V-SCAN017266/19)","2019-01-22T23:59:35","","Completed","2019-01-22T23:59:35","No","No","No","Internal"]
[null,null,null,183,null,"45_Mon Oct 07 2019 04:47:07 GMT+0000","2019-01-27T23:59:35","Defect","Ship Staff","Ship Staff Insp.","AE#2 auto start malfunctioning. AE#2 starting in auto except when it is in block condition ,while AE#3 starting/running ","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Hyundai technician attended job at Singapore on 14/03/2019 . Found short circuit on cable from instrument panel to junction box. Same to be renewed. Temporarily shorting cables disconnected. Plan to swap the cable between No 1 & No 2 AE and test (18 Mar 2019). Spare cable to be arranged through Hyundai. Reqn pending.","2019-05-31T23:59:35","SCAN190058","Completed","2019-07-09T23:59:35","No","No","No","Internal"]
[null,null,null,184,null,"45_Sat Oct 05 2019 23:54:50 GMT+0000","2019-02-03T23:59:35","Defect","Ship Staff","Ship Staff Insp.","STBD Bridge Wing Rudder Angle Indicator Dimmer Not Working","Navigation - Others","","Equipment Related","8.12","Medium","","","Renewed with new spare PCB ,working satisfactory.unplaned job order no : V-SCAN018052/19","2019-03-07T23:59:35","SCAN190013","Completed","2019-03-12T23:59:35","No","No","No","Internal"]
[null,null,null,185,null,"45_Sat Oct 05 2019 23:46:18 GMT+0000","2019-02-10T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Angle indcator units for Port & Stbd gangways found damaged","Deck - Pipe / Fittings","General Appearance","Equipment Related","5.47","Medium","","","Fabricated new angle indicator units and renewed for both Port and Stbd gangways.","2019-02-15T23:59:35","","Completed","2019-02-13T23:59:35","No","No","No","Internal"]
[null,null,null,186,null,"45_Sat Oct 05 2019 23:33:31 GMT+0000","2019-02-12T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Deck seal water pressure switch found defective and giving alarm","Inert Gas","Cargo / Ballast Systems","Equipment Related","8.35","Medium","","","Renewed with new pressure switch of same range . RO raised for spare. JOB ORDER NO: (V-SCAN017516/19)","2019-02-16T23:59:35","SCAN190020","Completed","2019-02-12T23:59:35","No","No","No","Internal"]
[null,null,null,187,null,"45_Sat Oct 05 2019 23:39:08 GMT+0000","2019-02-12T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Analyse Pump for Fix gas detection systm for ballast tank giving abnormal sound.","Miscellaneous","Cargo / Ballast Systems","Equipment Related","5.21","Medium","","","Pump overhauled and Pump Diaphragm renewed. Pump tested and working satisfactory.JOB ORDER NO :(V-SCAN017523/19)","2019-02-15T23:59:35","","Completed","2019-02-12T23:59:35","No","No","No","Internal"]
[null,null,null,188,null,"45_Sun Oct 06 2019 00:22:06 GMT+0000","2019-02-13T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Acetylene pipe line above paint locker found with material wastage and holed at clamping area","Deck - Pipe / Fittings","General Appearance","Equipment Related","5.26","Medium","","","Wasted section renewed. System tested for leakage and found satisfactory.","2019-03-21T23:59:35","","Completed","2019-03-26T23:59:35","No","No","No","Internal"]
[null,null,null,189,null,"45_Sat Oct 05 2019 23:51:08 GMT+0000","2019-02-21T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Ullage and IG pressure feed not displayed for 1S COT in SAAB Radar console in CCR","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.12","Medium","","","SAAB radar cover opened for 1S COT, found ingress of water. Same cleaned. Wire found core found broken in TGU unit. Same repaired.Working satisfactory now","2019-02-28T23:59:35","","Completed","2019-02-23T23:59:35","No","No","No","Internal"]
[null,null,null,190,null,"45_Sun Oct 06 2019 19:06:37 GMT+0000","2019-02-26T23:59:35","Defect","Ship Staff","Ship Staff Insp.","At middle part of the Port gangway (joint) found some wastage (holes) on the gangway frame body due to corrosion.","Deck - Machinery","General Appearance","Equipment Related","5.47","Medium","","","Wastage built up by steel putty and boxed back. Permanent job to be done at DD. Shall include in Refman. Included in DD spec. REFMAN Export ID: SDR 16 DK.18 09-MAR-2019","2019-02-28T23:59:35","","Completed","2019-06-14T23:59:35","No","No","No","Internal"]
[null,null,null,9426,null,"45_03/01/2020 8:33:15 PM","2019-03-09T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","dynamic data in AIS was not updated to \"moored\" after vessel's berthing","Navigation - GMDSS & Communication","Navigation","Behaviour Based,Human Error","","","","","dynamic data updated","2019-04-15T23:59:35","","Completed","2019-03-09T23:59:35","No","No","No","Internal"]
[null,null,null,9427,null,"45_03/01/2020 8:38:44 PM","2019-03-09T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","The Non WGS 84 Datum Chart in South China Sea after Eastern Bank was not identified and noted in the passage plan for the voyage","Navigation - ECDIS","Navigation","Behaviour Based,Human Error","4.2","Medium","","","The Passage Plan was amended and the Non WGS 84 Datum Chart in South China Sea after Eastern Bank was noted in the passage plan for the voyage","2019-03-09T23:59:35","","Completed","2019-03-09T23:59:35","No","No","No","Internal"]
[null,null,null,191,null,"45_Sun Oct 06 2019 00:10:54 GMT+0000","2019-03-17T23:59:35","Defect","Ship Staff","Ship Staff Insp.","AUS discharge valves of COPT #1, 2 & 3 not responding suitably for AUTO unloading operation.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.11","Medium","","","Valve positioners of all three COPs calibrated and set for AUTO unloading operation.","2019-03-21T23:59:35","","Completed","2019-03-19T23:59:35","No","No","No","Internal"]
[null,null,null,192,null,"45_Mon Oct 07 2019 02:57:16 GMT+0000","2019-03-22T23:59:35","Defect","Ship Staff","Ship Staff Insp.","ECR fwd HVAC unit ineffective cooling. Low sucn press and high dish pressures noticed.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Dryer found defective. New dryer fitted and system put to service and found satisfactory.","2019-03-28T23:59:35","","Completed","2019-03-24T23:59:35","No","No","No","Internal"]
[null,null,null,193,null,"45_Mon Oct 07 2019 03:09:52 GMT+0000","2019-03-23T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Leakage from FWG seawater piping. A section of pipe found wasted.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.31","Very High","","","Wasted section of pipe renewed and system put to service and found good.","2019-03-31T23:59:35","","Completed","2019-03-31T23:59:35","No","No","No","Internal"]
[null,null,null,195,null,"45_Mon Oct 07 2019 03:03:04 GMT+0000","2019-03-31T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Emg gen engine RPM indicator needle did not reflect the actual engine rpm.","Critical Equip.,Elect. Mach. & Equip.","Emgcy. Systems","Equipment Related","10.32","Very High","","","Cables cleaned and retightened and found indicator working normal","2019-03-31T23:59:35","","Completed","2019-03-31T23:59:35","No","No","No","Internal"]
[null,null,null,196,null,"45_Mon Oct 07 2019 03:12:38 GMT+0000","2019-04-03T23:59:35","Defect","Ship Staff","Ship Staff Insp.","#1 FWG condenser outlet line holed.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Pipe line to remove and fabricate new one.","2019-04-09T23:59:35","","Completed","2019-04-05T23:59:35","No","No","No","Internal"]
[null,null,null,197,null,"45_Sun Oct 06 2019 00:25:13 GMT+0000","2019-04-14T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Crew laundry drier not working.Bush got damaged","Miscellaneous","MLC Related","Equipment Related","11.16","Low","","","Bush fabricated and renewed.","2019-04-29T23:59:35","","Completed","2019-04-27T23:59:35","No","No","No","Internal"]
[null,null,null,198,null,"45_Sun Oct 06 2019 23:24:55 GMT+0000","2019-04-14T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Ship Staff Insp.","Stbd provision crane luffing cylinder top cover, hyd leak.","Deck - Machinery","Mooring","Equipment Related","8.76","Medium","","","Seal renewed. Tested and found satisfactory.","2019-06-30T23:59:35","SCAN190083","Completed","2019-07-12T23:59:35","No","No","No","Internal"]
[null,null,null,9424,null,"45_03/01/2020 8:25:32 PM","2019-04-15T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Accom. found to be in slight vacuum during cargo operations","E/R - Air Comp.,Miscellaneous","ISM Related","Human Error","5.1","Very High","","","Accom. pressure adjusted to maintain positive pressure inside accomodation","2019-04-15T23:59:35","","Completed","2019-04-15T23:59:35","No","No","No","Internal"]
[null,null,null,9425,null,"45_03/01/2020 8:30:02 PM","2019-04-15T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","1 VHF on bridge was found on 25W instead of 1W","Navigation - GMDSS & Communication","Communication","Behaviour Based,Human Error","","","","","VHF powered down to 1W","2019-04-15T23:59:35","","Completed","2019-04-15T23:59:35","No","No","No","Internal"]
[null,null,null,9428,null,"45_03/01/2020 8:18:38 PM","2019-04-15T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Training of jr. Officer in equipments for temperature & pressure calibration to be carrie dout","Miscellaneous","Cargo / Ballast Systems","Behaviour Based,Human Error,Knowledge Based","8.26","High","","","pressure & temperature calibration training given to junior officers","2019-04-30T23:59:35","","Completed","2019-04-20T23:59:35","No","No","No","Internal"]
[null,null,null,199,null,"45_Mon Oct 07 2019 03:20:06 GMT+0000","2019-04-16T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Sucn Pipe line choked.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Removed pipe section. Cleared the obstruction and fitted back.","2019-04-28T23:59:35","","Completed","2019-04-24T23:59:35","No","No","No","Internal"]
[null,null,null,200,null,"45_Sun Oct 06 2019 19:02:34 GMT+0000","2019-04-21T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Port windlass, brake cyl hyd leak from bottom & top cover.","Deck - Mooring Machinery","Mooring","Equipment Related","9.14","Medium","","","Seal ring renewed. System tested and found satisfactory.","2019-06-17T23:59:35","","Completed","2019-06-04T23:59:35","No","No","No","Internal"]
[null,null,null,201,null,"45_Sun Oct 06 2019 00:27:39 GMT+0000","2019-04-24T23:59:35","Defect","Ship Staff","Ship Staff Insp.","No 3 COP NRV suspected to malfunction.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.11","Medium","","","NRV inspected and found free. PAL JO: V-SCAN018857/19","2019-05-01T23:59:35","","Completed","2019-04-24T23:59:35","No","No","No","Internal"]
[null,null,null,202,null,"45_Sun Oct 06 2019 23:50:59 GMT+0000","2019-04-24T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Stbd hose crane, jerky during luffing operation","Deck - Machinery","Mooring","Equipment Related","8.76","Medium","","","Fulcrum pins to be lubricated. Crane to be operated and checked. Grease applied through lubrication points. Vibration has reduced. In communication with service provider. Crane luff cyl control valve spool inspected and found normal. Greasing routine repeated. Movement observed to be better. Need to operate onload and check. Job included in Refman DD spec.","2019-07-30T23:59:35","","Completed","2019-07-31T23:59:35","No","No","No","Internal"]
[null,null,null,203,null,"45_Sun Oct 06 2019 19:09:18 GMT+0000","2019-04-28T23:59:35","Defect","Ship Staff","Ship Staff Insp.","No 1 COP AUS discharge valve positioner defective.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.11","Medium","","","Feedback linkage to positioner found disconnected. Same fitted and calibrated. Found satisfactory","2019-06-05T23:59:35","","Completed","2019-06-03T23:59:35","No","No","No","Internal"]
[null,null,null,204,null,"45_Mon Oct 07 2019 00:58:18 GMT+0000","2019-05-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","DGPS PRINTER NOT OPREATIONAL","Navigation - DGPS / EPFS / AIS","Navigation","Equipment Related","4.7","High","","","NEED TO REPLACE THE PRINTER . ( PRINTER HEAD WAS CHANGED AFTER RECEIVING THE SPARE BUT ISSUE NOT SOLVED. NEED TO REPLACE PRINTER UNIT )","2019-08-25T23:59:35","SCAN190093","Completed","2019-08-24T23:59:35","No","No","No","Internal"]
[null,null,null,205,null,"45_Mon Oct 07 2019 03:23:42 GMT+0000","2019-05-03T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Main Air Compressor #2, 2nd stage cyl head stud cracked.","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Compressor inspected. Cracked stud replaced with spare new stud. Tried out and found satisfactory.","2019-05-04T23:59:35","","Completed","2019-05-04T23:59:35","No","No","No","Internal"]
[null,null,null,206,null,"45_Sun Oct 06 2019 00:30:17 GMT+0000","2019-05-08T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Oil leakage from Aft winch hyd control valve block","Deck - Mooring Machinery","Mooring","Equipment Related","9.14","Medium","","","Control valve block removed. Seals renewed. Winch tested and found satisfactory.","2019-05-15T23:59:35","","Completed","2019-05-10T23:59:35","No","No","No","Internal"]
[null,null,null,207,null,"45_Mon Oct 07 2019 03:30:59 GMT+0000","2019-05-13T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Main air compressor #2, Performance below normal.","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","1st and 2nd stage valves inspected. 2nd stage discharge valve plate found broken. Valve overhauled with new spare. Compressor tried out and found satisfactory.","2019-05-14T23:59:35","V-SCAN019477/19","Completed","2019-05-14T23:59:35","No","No","No","Internal"]
[null,null,null,208,null,"45_Mon Oct 07 2019 03:34:06 GMT+0000","2019-05-17T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Pin hole in Seawater piping, soot tank eductor line.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Pipe removed to workshop. Leaky section renewed and fitted back. Tested and found satisfactory.","2019-05-18T23:59:35","V-SCAN019478/19","Completed","2019-05-18T23:59:35","No","No","No","Internal"]
[null,null,null,209,null,"45_Mon Oct 07 2019 03:37:29 GMT+0000","2019-05-24T23:59:35","Defect","Ship Staff","Ship Staff Insp.","AE #1, unit 6 exh temp dropped during operation. ","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Upon trouble shooting found the fuel injector defective. Replaced with spare fuel injector. Tested and found satisfactory.","2019-05-25T23:59:35","V-SCAN019479/19","Completed","2019-05-25T23:59:35","No","No","No","Internal"]
[null,null,null,210,null,"45_Mon Oct 07 2019 03:43:18 GMT+0000","2019-05-27T23:59:35","Defect","Ship Staff","Ship Staff Insp.","FWG Ejector pump shaft seal leaking","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Pump overhauled, seal renewed and tested. Found satisfactory.","2019-05-28T23:59:35","V-SCAN019480/19","Completed","2019-05-27T23:59:35","No","No","No","Internal"]
[null,null,null,211,null,"45_Mon Oct 07 2019 03:48:25 GMT+0000","2019-05-29T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Main & COPT #3 cool SW pump shaft seal leaking.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Shaft seal renewed with spare.","2019-06-05T23:59:35","V-SCAN019802/19","Completed","2019-06-03T23:59:35","No","No","No","Internal"]
[null,null,null,212,null,"45_Sun Oct 06 2019 19:19:06 GMT+0000","2019-05-30T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Fwd spring winch  hyd return line corroded.","Deck - Mooring Machinery","Mooring","Equipment Related","9.14","Medium","","","Oil drained, Section of pipe removed and Shifted to Engine room workshop. Section of pipe cropped and renewed. System tested and found no leak.","2019-06-10T23:59:35","","Completed","2019-06-01T23:59:35","No","No","No","Internal"]
[null,null,null,213,null,"45_Sun Oct 06 2019 19:31:32 GMT+0000","2019-05-30T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Stbd side Gangway securing arrangement found broken","Deck - Machinery","General Appearance","Equipment Related","5.47","Medium","","","permanent repair carried out. ","2019-06-30T23:59:35","","Completed","2019-06-27T23:59:35","No","No","No","Internal"]
[null,null,null,214,null,"45_Sun Oct 06 2019 19:34:32 GMT+0000","2019-05-30T23:59:35","Defect","Ship Staff","Ship Staff Insp.","3 COT no.2 Cow machine found not rotating during cow wash at last discharge port","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.34","High","","","Machine need to be taken out and overhaul & box back. Overhauled and found satisfactory.","2019-06-30T23:59:35","","Completed","2019-06-24T23:59:35","No","No","No","Internal"]
[null,null,null,215,null,"45_Sun Oct 06 2019 19:42:49 GMT+0000","2019-05-30T23:59:35","Defect","Ship Staff","Ship Staff Insp.","4 Port COT no.1 Cow machine drive unit found during cow wash not rotating as per maker","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.34","High","","","It has been planned to over haul Drive unit & box back on passage. Overhauled and found satisfactory.","2019-06-30T23:59:35","","Completed","2019-06-25T23:59:35","No","No","No","Internal"]
[null,null,null,216,null,"45_Mon Oct 07 2019 04:41:05 GMT+0000","2019-06-02T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Galley hot plate low IR","Elect. Mach. & Equip.","General Appearance","Equipment Related","11.16","Low","","","Galley hot plates dismantled to check the condition of wires and switch , brittle wires changed with spare , Hot plate IR measured found below 3 mega ohms . Due to low IR 440 low insulation alarm is getting activated , need to replace with spare . RO SCAN190102","2019-06-30T23:59:35","V-SCAN020093/19","Completed","2019-07-06T23:59:35","No","No","No","Internal"]
[null,null,null,217,null,"45_Sun Oct 06 2019 18:56:59 GMT+0000","2019-06-03T23:59:35","Defect","Ship Staff","Ship Staff Insp.","VDR error","Navigation - VDR / BNWAS","Navigation","Equipment Related","4.7","High","","","VDR error observed was coming due to alarm in the system same rectified working satisfcactory","2019-06-04T23:59:35","","Completed","2019-06-04T23:59:35","No","No","No","Internal"]
[null,null,null,218,null,"45_Mon Oct 07 2019 03:45:42 GMT+0000","2019-06-03T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Hydraphore pipe outlet to engine room found crack","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.31","Very High","","","Pipe section renewed","2019-06-10T23:59:35","V-SCAN019801/19","Completed","2019-06-05T23:59:35","No","No","No","Internal"]
[null,null,null,219,null,"45_Sun Oct 06 2019 23:27:53 GMT+0000","2019-06-03T23:59:35","Defect","Ship Staff","Ship Staff Insp.","FIXED GAS Detection system internal leakage ","Miscellaneous","Cargo / Ballast Systems","Equipment Related","5.21","Medium","","","Pumps overhauled with spare kit. Tested and found satisfactory.","2019-07-15T23:59:35","SCAN190103","Completed","2019-07-15T23:59:35","No","No","No","Internal"]
[null,null,null,220,null,"45_Sun Oct 06 2019 19:00:02 GMT+0000","2019-06-04T23:59:35","Defect","Ship Staff","Ship Staff Insp.","COT NO -5P PRESSURE ERROR ","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.12","Medium","","","COT NO -5P PRESSURE ERROR and eratic readings were coming on display same rectified by dismantaling the pressure sensor; cleaned calibrated and fitted back, working satisfactory ","2019-06-07T23:59:35","V-SCAN019822/19","Completed","2019-06-07T23:59:35","No","No","No","Internal"]
[null,null,null,221,null,"45_Sun Oct 06 2019 19:22:08 GMT+0000","2019-06-13T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Forward air whistle not working","Navigation - Others","Navigation","Equipment Related","4.7","High","","","Whistle inspected and spares kept ready. Working Satisfactory","2019-06-25T23:59:35","V-SCAN019958/19","Completed","2019-06-26T23:59:35","No","No","No","Internal"]
[null,null,null,222,null,"45_Mon Oct 07 2019 08:18:49 GMT+0000","2019-06-13T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Forward Air whistle not working","Navigation - Others","Navigation","Equipment Related","4.7","High","","","Whistle inspected and spares kept ready.","2019-06-25T23:59:35","V-SCANNO19958/19","Completed","2019-06-26T23:59:35","No","No","No","Internal"]
[null,null,null,223,null,"45_Wed Jul 10 2019 05:20:40 GMT+0000","2019-06-13T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","60% LT Cooler inlet elbow stub piece corroded","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Stub piece to renew. At present cold repair carried out. Cooler need to be drained for repairs. Job shall be attended in ballast passage.","2019-07-10T23:59:35","V-SCAN020263/19","Completed","2019-07-13T23:59:35","No","No","No","Internal"]
[null,null,null,224,null,"45_Mon Oct 07 2019 03:56:51 GMT+0000","2019-06-16T23:59:35","Defect","Ship Staff","Ship Staff Insp.","#2 Boiler FO pump seal found leaking","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Pump to overhaul.","2019-06-24T23:59:35","V-SCAN001481/18","Completed","2019-06-22T23:59:35","No","No","No","Internal"]
[null,null,null,225,null,"45_Mon Oct 07 2019 06:00:53 GMT+0000","2019-06-17T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Atmospheric condensor sea wateroutlet pipe found pin hole","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","External Factors","10.32","Very High","","","Temporary repair done. Awaiting anchorage to do permant repair. DD spec made.","2019-07-25T23:59:35","DD SPEC","Completed","2019-07-25T23:59:35","Yes","No","No","Internal"]
[null,null,null,226,null,"45_Mon Oct 07 2019 05:29:45 GMT+0000","2019-06-19T23:59:35","Defect","Ship Staff","Ship Staff Insp.","STBD waste water pipe storm valve defective. Pin hole in attached pipe","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","External Factors","10.32","Very High","","","STORM VALVE RENEWED WITH NEW SPARE. Pinhole welded and repaired","2019-07-06T23:59:35","V-SCAN020265/19","Completed","2019-07-06T23:59:35","No","No","No","Internal"]
[null,null,null,227,null,"45_Mon Oct 07 2019 05:27:17 GMT+0000","2019-06-20T23:59:35","Defect","Ship Staff","Ship Staff Insp.","GALLEY DRAIN OVERBOARD STORM VALVE BODY LEAKING. VALVE TO RENEW.","E/R - Pipes/ valves & fittings","","External Factors","6.4","High","","","STORM VALVE RENEWED WITH NEW SPARE","2019-07-06T23:59:35","V-SCAN020264/20","Completed","2019-07-07T23:59:35","No","No","No","Internal"]
[null,null,null,228,null,"45_Mon Oct 07 2019 04:00:42 GMT+0000","2019-06-22T23:59:35","Defect","Ship Staff","Ship Staff Insp.","PORT SIDE BRIDGE WING CAMERA HORIZONENTAL DISTORTION NOTICED ON THE SCREEN AND FLICKERING","Elect. Mach. & Equip.,Miscellaneous","Navigation","Equipment Related","11.16","Low","","","CAMERA DISMENTALED CHECKED FOR LOOSE CONNECTIONS ALL INTACT, FOUND NO BURNED PARTS ON PCB. SYSTEM RESTARTED AFTER CHECKS BUT SAME CONDITION , NEED OFFICE ADVICE ","2019-06-30T23:59:35","","Completed","2019-06-25T23:59:35","No","No","No","Internal"]
[null,null,null,229,null,"45_Mon Oct 07 2019 05:43:18 GMT+0000","2019-06-26T23:59:35","Defect","Ship Staff","Ship Staff Insp.","FWG-2  Distallate pump moror windings found open ckt.","E/R - Aux. Mach.","Eng. / Strg. Comp.","External Factors","10.32","Very High","","","Fabricating a spacer ring to fit the motor to the pump flange. Job in progress. ","2019-07-14T23:59:35","","Completed","2019-07-17T23:59:35","No","No","No","Internal"]
[null,null,null,230,null,"45_Mon Oct 07 2019 00:59:51 GMT+0000","2019-06-29T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Telegraph printer not printing properly","Navigation - Others","Navigation","Equipment Related","4.7","High","","","Movement started logging down in Bridge Bell Book and Req has been raised for defect item.","2019-08-25T23:59:35","SCAN190128","Completed","2019-07-24T23:59:35","No","No","No","Internal"]
[null,null,null,231,null,"45_Mon Oct 07 2019 00:12:33 GMT+0000","2019-06-30T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","5P ballast tank valve indication needle overshoots full open posn and falls to zero position when valve is actually full open.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.13","Medium","","","Local indicator opened up for wrong signal found normal working in range as there is mechanical stopper for the needle. Electronic indicator stop overshooting after adjusting from the PCB and dial adjuster below the indicator. ","2019-08-25T23:59:35","","Completed","2019-08-12T23:59:35","No","No","No","Internal"]
[null,null,null,266,null,"45_Sun Oct 06 2019 23:49:00 GMT+0000","2019-07-06T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","WO Sludge tk, Bilge tank – save all edges corroded/wasted","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","External Factors","6.9","Low","","","Included in REFFMA to carry out at DD","2019-07-19T23:59:35","","Completed","2019-07-19T23:59:35","No","No","No","Internal"]
[null,null,null,173,null,"45_Wed Jul 10 2019 02:02:39 GMT+0000","2019-07-06T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Hose crane Emergency pump for Hoist/Luff operation missing, emergency procedures not tried out","Deck - Machinery","Mooring","Equipment Related","8.5","Very High","","","Spare recieved & closed out","2019-12-30T23:59:35","SCAN190177","Completed","2019-12-25T23:59:35","No","No","No","Internal","Will be supplied in Singapore. Target date revised due to lead time of spares."]
[null,null,null,179,null,"45_Mon Oct 07 2019 05:08:42 GMT+0000","2019-07-06T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ER arrival checklist not updated and signed – pages found blank","Miscellaneous","Eng. / Strg. Comp.","External Factors,Human Error","4.3","Medium","","","Checklists are supposed to be diligently followed and updated and it’s a NC – for not following SMS procdures","2019-07-12T23:59:35","","Completed","2019-07-06T23:59:35","No","No","No","Internal"]
[null,null,null,232,null,"45_Mon Oct 07 2019 04:53:26 GMT+0000","2019-07-06T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Aft engine pit dirty and oily","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.19","Very High","","","To clean, check source of leakage and maintain clean.Cleaned and made dry.","2019-08-12T23:59:35","","Completed","2019-07-07T23:59:35","No","No","No","Internal"]
[null,null,null,233,null,"45_Mon Oct 07 2019 08:28:37 GMT+0000","2019-07-06T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ER arrival Checklist not updated and signed pages found blank\t\t","Documentation","Cert. & Docu.","Human Error","8.104","Low","","","Checklist are supposed to be diligently followed and updated and its a NC for not following","2019-07-12T23:59:35","","Completed","2019-07-06T23:59:35","No","No","No","Internal"]
[null,null,null,234,null,"45_Mon Oct 07 2019 05:14:38 GMT+0000","2019-07-06T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp."," CFW cooler Inlet elbow leaking from connection pipe weld seam","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related,External Factors","10.32","Very High","","","To plan for welding repairs at suitable opportunity","2019-09-12T23:59:35","V-SCAN020263/19","Completed","2019-07-13T23:59:35","No","No","No","Internal"]
[null,null,null,235,null,"45_Sun Oct 06 2019 21:28:41 GMT+0000","2019-07-06T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","No spare foam nozzle retaining springs","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.35","Medium","","","Vessel have spare  4 sets","2019-07-26T23:59:35","","Completed","2019-07-07T23:59:35","No","No","No","Internal"]
[null,null,null,236,null,"45_Sun Oct 06 2019 21:34:02 GMT+0000","2019-07-06T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","IG drain line has soft patch","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","11.4","Very High","","","If opening flange to flange section is not possible, then to include in REFFMAN - Shifted to REFMAN","2019-07-26T23:59:35","","Completed","2019-07-11T23:59:35","No","No","No","Internal"]
[null,null,null,237,null,"45_Mon Oct 07 2019 05:33:07 GMT+0000","2019-07-06T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Control air line to LT cooler 3 way valve actuator cylinder leaking","E/R - Aux. Engine","Eng. / Strg. Comp.","External Factors","10.32","Very High","","","To check and rectify. //Gasket renewed.","2019-07-12T23:59:35","","Completed","2019-07-14T23:59:35","No","No","No","Internal"]
[null,null,null,238,null,"45_Mon Oct 07 2019 05:35:05 GMT+0000","2019-07-06T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","FO heater #1, steam line outlet steam trap leaking from gasket","E/R - Main Engine","Eng. / Strg. Comp.","External Factors","10.32","Very High","","","To rectify the leakage. Replaced gasket and rectified","2019-07-26T23:59:35","","Completed","2019-07-15T23:59:35","No","No","No","Internal"]
[null,null,null,239,null,"45_Mon Oct 07 2019 05:37:31 GMT+0000","2019-07-06T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","1 Frdge compressor running with sump oil level low","E/R - Aux. Mach.","Eng. / Strg. Comp.","External Factors","10.32","Very High","","","To top up oil to correct level. // Topped up.","2019-07-19T23:59:35","","Completed","2019-07-07T23:59:35","No","No","No","Internal"]
[null,null,null,240,null,"45_Mon Oct 07 2019 05:40:04 GMT+0000","2019-07-06T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Incinerator Noticed wrapped with cloth on sludge burner pump","E/R - Aux. Mach.","Eng. / Strg. Comp.","External Factors","10.32","Very High","","","Gaskets renewed. No leak observed.","2019-07-26T23:59:35","","Completed","2019-07-15T23:59:35","No","No","No","Internal"]
[null,null,null,241,null,"45_Sun Oct 06 2019 23:32:14 GMT+0000","2019-07-06T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","WBT valves opening hyd line on deck – cross deck line support back plates are wasted at few locations","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.5","Medium","","","To include in REFFMAN, to carry out at DD -Shifted to REFMAN","2019-08-12T23:59:35","","Completed","2019-07-15T23:59:35","No","No","No","Internal"]
[null,null,null,242,null,"45_Sun Oct 06 2019 23:41:08 GMT+0000","2019-07-06T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","2 foam monitor, gun/nozzle retaining spring, hanging looses, broken form support base","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.35","Medium","","","Retaining spring has been replace","2019-07-26T23:59:35","","Completed","2019-07-24T23:59:35","No","No","No","Internal"]
[null,null,null,243,null,"45_Sun Oct 06 2019 23:44:09 GMT+0000","2019-07-06T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Few Hyd return lines were reported renewed recently, as same was wasted","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.5","Medium","","","Wasted section Welded with doubler and fitted back, same has been enter in Refman for Permanent renewal","2019-08-12T23:59:35","","Completed","2019-07-26T23:59:35","No","No","No","Internal"]
[null,null,null,244,null,"45_Sun Oct 06 2019 23:46:11 GMT+0000","2019-07-06T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Gangway Lubricator and moisture drain filters seems not carried out – covers were seized","Deck - Machinery","General Appearance","Equipment Related","5.47","Medium","","","Gangway Lubricator and moisture drain filters cleaned/overhaul and box back","2019-07-26T23:59:35","","Completed","2019-07-26T23:59:35","No","No","No","Internal"]
[null,null,null,245,null,"45_Mon Oct 07 2019 05:56:26 GMT+0000","2019-07-06T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Noticed, Deep Freezer for wet garbage kept in dry provision room","Miscellaneous","Eng. / Strg. Comp.","External Factors","10.32","Very High","","","Discussed with Supt as there is no issue for Deep Freezer in present location.","2019-07-19T23:59:35","","Completed","2019-07-19T23:59:35","No","No","No","Internal"]
[null,null,null,246,null,"45_Mon Oct 07 2019 05:59:03 GMT+0000","2019-07-06T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","WO Sludge tk, Bilge tank – save all edges corroded/wasted","Deck - Machinery","Eng. / Strg. Comp.","External Factors","10.32","Very High","","","Included in REFFMA to carry out at DD","2019-07-19T23:59:35","","Completed","2019-07-19T23:59:35","Yes","No","No","Internal"]
[null,null,null,247,null,"45_Sun Oct 06 2019 23:52:56 GMT+0000","2019-07-06T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Steering flat/storage COT, various valve seat rings lying open in cardboard box – prone to heat and damage","Miscellaneous","Cargo / Ballast Systems","Human Error","10.29","Medium","","","To shift to any stores inside accommodation to avoid damage to seat rings, to take inventory of seat rings and maintain list/update PAL. Shifted.","2019-07-26T23:59:35","","Completed","2019-07-18T23:59:35","No","No","No","Internal"]
[null,null,null,248,null,"45_Mon Oct 07 2019 08:38:27 GMT+0000","2019-07-06T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Steering flat/Stowage COT , various valve seat rings lying open in cardboard box\t","Miscellaneous","Eng. / Strg. Comp.","Human Error","10.29","Medium","","","to shift to any store inside accomodation to avoid damage to seat rings, to take inventory","2019-07-26T23:59:35","","Completed","2019-07-18T23:59:35","No","No","No","Internal"]
[null,null,null,249,null,"45_Sun Oct 06 2019 23:56:19 GMT+0000","2019-07-06T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Pumproom Blower damper remote operation cabinet corroded/wasted","Deck - Machinery","General Appearance","External Factors","5.19","Medium","","","Shifted to REFFMAN","2019-07-31T23:59:35","","Completed","2019-07-31T23:59:35","No","No","No","Internal"]
[null,null,null,250,null,"45_Mon Oct 07 2019 06:02:26 GMT+0000","2019-07-06T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","2 FW cooler SW outletconnection flange piece considerable sea water leakage observed","E/R - Aux. Engine","Eng. / Strg. Comp.","External Factors","10.32","Very High","","","To check/remove intermediate section, renew gasket as necessary. Planned for next ballast passage.","2019-09-12T23:59:35","V-SCAN020696/19","Completed","2019-08-06T23:59:35","No","No","No","Internal"]
[null,null,null,251,null,"45_Mon Oct 07 2019 06:06:33 GMT+0000","2019-07-06T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","IGG sea water line filter casing holed and leaking","Inert Gas","Eng. / Strg. Comp.","External Factors","8.3","Very High","","","To remove the casing weld/repair and fit back","2019-08-15T23:59:35","V-SCAN020696/19","Completed","2019-08-08T23:59:35","No","No","No","Internal"]
[null,null,null,252,null,"45_Mon Oct 07 2019 00:55:15 GMT+0000","2019-07-06T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Near Helicopter area, on deck, observed coating damage and paint peel off around/abt 30 sq mtrs area","Miscellaneous","General Appearance","External Factors","11.3","Medium","","","Improper surface preparation, waste of paints – to ensure proper procedure is followed while paint application","2019-08-15T23:59:35","","Completed","2019-08-15T23:59:35","No","No","No","Internal"]
[null,null,null,253,null,"45_Mon Oct 07 2019 01:01:46 GMT+0000","2019-07-06T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Stores/Space spaces Lying haphazard and doesn’t look organized","Miscellaneous","General Appearance","Human Error","5.11","Low","","","To utlize the next long Voyage, to take inventory, update and arrange/organize orderly. Stores and spares neatly arranged.","2019-07-26T23:59:35","","Completed","2019-07-28T23:59:35","No","No","No","Internal"]
[null,null,null,254,null,"45_Mon Oct 07 2019 06:08:38 GMT+0000","2019-07-06T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Control air dryer Defective/In-operational","E/R - Air Comp.","Eng. / Strg. Comp.","External Factors","10.32","Very High","","","New unit INSTALLED AND COMMISSSIONED","2019-09-05T23:59:35","","Completed","2019-09-03T23:59:35","No","No","No","Internal"]
[null,null,null,255,null,"45_Wed Jul 10 2019 06:12:18 GMT+0000","2019-07-06T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Aux Engines Not fitted with Oil max filters yet","E/R - Aux. Engine","Eng. / Strg. Comp.","External Factors","10.32","Very High","","","Fitted for all three DG's  and working satisfactory","2019-09-03T23:59:35","","Completed","2019-09-07T23:59:35","No","No","No","Internal"]
[null,null,null,256,null,"45_Sun Oct 06 2019 19:48:03 GMT+0000","2019-07-10T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","All winch brake band adjusting bolt clearances were not as per maker’s reccommendation","Deck - Mooring Machinery","Mooring","Equipment Related","9.14","Medium","","","Adjusted as per recommended clearance requiered.","2019-07-19T23:59:35","","Completed","2019-07-10T23:59:35","No","No","No","Internal"]
[null,null,null,175,null,"45_Wed Jul 10 2019 02:09:03 GMT+0000","2019-07-10T23:59:35","Defect","Ship Staff","Ship Staff Insp.","5P I.G pressure not showing on SAAB radar screen","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.13","Medium","",""," Pressure sensor  renewed.  Working satisfactory","2019-12-30T23:59:35","SCAN190136","Completed","2019-12-30T23:59:35","No","No","No","Internal","Will be supplied in Singapore.I will be carrying spares with me to Qingdao. Target date revised due to lead time of spares."]
[null,null,null,176,null,"45_Wed Jul 10 2019 02:11:44 GMT+0000","2019-07-16T23:59:35","Defect","Ship Staff","Ship Staff Insp.","5C C.O.T level and I.G pressure not showing on SAAB radar screen and Loadicator","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.13","Medium","",""," TGE unit and Pressure sensor renewed, working satisfactory.","2019-12-30T23:59:35","SCAN190136","Completed","2019-12-30T23:59:35","No","No","No","Internal","I will be carrying spares with me to Qingdao. Target date revised due to lead time of spares."]
[null,null,null,257,null,"45_Mon Oct 07 2019 05:45:27 GMT+0000","2019-07-17T23:59:35","Defect","Ship Staff","Ship Staff Insp.","E/R QMI oil mist detector for Aux. Boiler in fault","Elect. Mach. & Equip.","Eng. / Strg. Comp.","External Factors","10.32","Very High","","","Detector dismentaled for repair cleaned and fitted back but no posstive result need to replace the detector RO SCAN190137","2019-08-15T23:59:35","SCAN190137","Completed","2019-07-18T23:59:35","No","No","No","Internal"]
[null,null,null,258,null,"45_Mon Oct 07 2019 05:48:58 GMT+0000","2019-07-22T23:59:35","Defect","Ship Staff","Ship Staff Insp.","MGPS LOW SEA CHEST CURRENT GETTING ZERO AFTER SETTING ANY VALUE ","Elect. Mach. & Equip.","Eng. / Strg. Comp.","External Factors","10.32","Very High","","","SYSTEM CHECKED FOR LOOSE CONNECTION FOUND ALL INTACT , SYSTEM RESTARTED BUT NO POSSITIVE RESULT , SUSPECTED POWER  AND CONTROL UNIT SAME OPENED AND REAPIRED SYSTEM WORKING SATISFACTORY  RO SCAN190139 MADE FOR FUTURE USE","2019-08-30T23:59:35","SCAN190139","Completed","2019-07-25T23:59:35","No","No","No","Internal"]
[null,null,null,10745,null,"45_04-Mar-20 12:23:35 PM","2019-08-01T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Ballast Sea Chest (BA 033) Valve Leaking","Cargo Mach.","Cargo / Ballast Systems","Equipment Related,External Factors","8.8","Medium","","","Seat ring to to be renewed. Vessel have spare seat ring onboard. Deferred to dry dock. Job created in REFMAN.","2020-08-31T23:59:35","","Completed","2020-07-22T23:59:35","Yes","No","No","Internal","Job to be shifted in Refman."]
[null,null,null,259,null,"45_Mon Oct 07 2019 00:01:24 GMT+0000","2019-08-03T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Seawater flusing valve found leaking","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.35","Medium","","","Replace valve with spare","2019-08-06T23:59:35","V-SCAN020688","Completed","2019-08-05T23:59:35","No","No","No","Internal"]
[null,null,null,260,null,"45_Mon Oct 07 2019 00:53:00 GMT+0000","2019-08-07T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Stbd side Gangway securing one arrangement found sheared","Deck - Machinery","General Appearance","Equipment Related","5.47","Medium","","","Sheared part permanently repaired and fix back","2019-08-15T23:59:35","","Completed","2019-08-13T23:59:35","No","No","No","Internal"]
[null,null,null,261,null,"45_Mon Oct 07 2019 06:10:28 GMT+0000","2019-08-17T23:59:35","Defect","Ship Staff","Ship Staff Insp.","SW leakage from #1 FWG eductor","E/R - Aux. Engine","Eng. / Strg. Comp.","External Factors","10.32","Very High","","","Eductor body found erroded. Need to replace. RO raised for spare SCAN190158. Repaired by brazing. ","2019-10-15T23:59:35","SCAN190158","Completed","2019-09-03T23:59:35","No","No","No","Internal"]
[null,null,null,8148,null,"45_16/12/2019 3:20:31 PM","2019-08-20T23:59:35","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Clean old oil stains near NO.1 boiler supply pump gland packing.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.19","Very High","","","Oil stain cleaned and painted","2019-09-24T23:59:35","","Completed","2019-09-22T23:59:35","No","No","No","Internal"]
[null,null,null,177,null,"45_Wed Jul 10 2019 06:26:06 GMT+0000","2019-09-15T23:59:35","Defect","Ship Staff","Ship Staff Insp.","QMI MIST DETECTOR AUX BOILER NO 1 NOT OPERATIONAL","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","5.35","Medium","","","QMI SENSOR REPLACED WITH NEW SPARE , WORKING SATISFACTORY","2019-12-30T23:59:35","SCAN190137","Completed","2019-12-27T23:59:35","No","No","No","Internal","Will be Supplied in singapore."]
[null,null,null,262,null,"45_Mon Oct 07 2019 01:08:04 GMT+0000","2019-09-18T23:59:35","Defect","PSC Insp.","PSC Inspection","The Last 1 meter of the Vapor piping upstream of the vapor connection must be painted Red/Yellow/Red. The Vapor control piping on board did not meet the required Color Scheme ","Deck - Pipe / Fittings","Cargo / Ballast Systems","Human Error","8.42","Medium","Cargo operations including equipment","","Red colour marking band of 100 mm as required were painted on the Vapour return line manifold same day of the observation.","2019-09-18T23:59:35","","Completed","2019-09-18T23:59:35","No","No","No","External"]
[null,null,null,263,null,"45_Mon Oct 07 2019 06:17:07 GMT+0000","2019-09-18T23:59:35","Defect","PSC Insp.","PSC Inspection","The condition of the ship’s equipment shall not present dangers to the ship or it’s crew. The gasket material around the incinerator door was deteriorated","Miscellaneous","Eng. / Strg. Comp.","External Factors","10.32","Very High","Other","","Replaced Gasket.","2019-09-18T23:59:35","","Completed","2019-09-19T23:59:35","No","No","No","External"]
[null,null,null,264,null,"45_Mon Oct 07 2019 06:15:33 GMT+0000","2019-09-18T23:59:35","Defect","PSC Insp.","PSC Inspection","The condition of the ship and its equipment shall be maintained to conform to the provisions of the current regulations & ensure the ship remains fit to proceed to sea w/o presenting dangers to the ship or persons. The refractory of the incinerator was degraded.","Miscellaneous","Eng. / Strg. Comp.","External Factors","10.32","Very High","Other","","Degraded refractory material restored with suitable refractory material","2019-09-18T23:59:35","","Completed","2019-09-19T23:59:35","No","No","No","External"]
[null,null,null,265,null,"45_Mon Oct 07 2019 01:10:28 GMT+0000","2019-09-18T23:59:35","Defect","PSC Insp.","PSC Inspection","The Tank Overfill alarm requires an audible & visible alarm. The Warning light was not visible during tests.","Elect. Mach. & Equip.","Cargo / Ballast Systems","Equipment Related","8.24","Medium","Alarms","","Replaced Bulb.","2019-09-18T23:59:35","","Completed","2019-09-18T23:59:35","No","No","No","External"]
[null,null,null,267,null,"45_Mon Oct 07 2019 02:00:46 GMT+0000","2019-09-19T23:59:35","Defect","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","The details relating to type and number of navigation equipment had not been completed within the OCIMF VPQ.","Documentation","Cert. & Docu.","Human Error","1.14","Low","","","The details updated in OCIMF VPQ.","2019-09-19T23:59:35","","Completed","2019-09-19T23:59:35","No","No","No","Internal"]
[null,null,null,268,null,"45_Mon Oct 07 2019 06:19:04 GMT+0000","2019-09-20T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","DECK SEAL PUMP #2 MECHANICAL SEAL LEAK","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","PUMP OVERHAULED, MECHANICAL SEAL RENEWED","2019-09-27T23:59:35","","Completed","2019-09-27T23:59:35","No","No","No","Internal"]
[null,null,null,269,null,"45_Mon Oct 07 2019 06:20:41 GMT+0000","2019-09-20T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","AE FO SUPPLY PUMP MECHANICAL SEAL LEAK","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","PUMP OVERHAULED AND MECHANICAL SEAL RENWED. PUMP PUT IN USE NO LEAKS FOUND","2019-09-27T23:59:35","","Completed","2019-09-24T23:59:35","No","No","No","Internal"]
[null,null,null,8092,null,"45_18/12/2019 3:23:34 PM","2019-09-20T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","UPS in steering gear room giving fault alarm","Elect. Mach. & Equip.","General Appearance","Equipment Related","11.1","High","","","UPS to be renewed.RO raaised","2020-09-30T23:59:35","SCAN 200006","Completed","2020-10-29T23:59:35","No","No","No","Internal"]
[null,null,null,8131,null,"45_16/12/2019 3:32:19 PM","2019-09-20T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Calorifier drain valve having minor leakge","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Leak rectified by tightening drain pipe","2019-09-24T23:59:35","","Completed","2019-09-24T23:59:35","No","No","No","Internal"]
[null,null,null,8132,null,"45_16/12/2019 2:41:48 PM","2019-09-20T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","A.E 2 Duplex filter having minor leakage","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.19","Very High","","","Duplex filter change over cock O- rings renewed, leak rectified.","2019-09-25T23:59:35","","Completed","2019-09-23T23:59:35","No","No","No","Internal"]
[null,null,null,8133,null,"45_16/12/2019 2:45:23 PM","2019-09-20T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","A.E 1 Fuel oil regulating valve having minor leakage","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.19","Very High","","","Ther is no leak, oil stain from fuel pipe, cleaned and painted.","2019-09-30T23:59:35","","Completed","2019-09-27T23:59:35","No","No","No","Internal"]
[null,null,null,8134,null,"45_16/12/2019 2:52:46 PM","2019-09-20T23:59:35","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","M.E jacket water piping behind FWG,2 flanges having salt deposits on it.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","",""," Salt deposits cleaned and painted","2019-09-24T23:59:35","","Completed","2019-09-23T23:59:35","No","No","No","Internal"]
[null,null,null,8135,null,"45_16/12/2019 2:57:49 PM","2019-09-20T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","M.E NO.4 unit lagging cover for exhaust manifold has become loose due to broken rivet","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.19","Very High","","","Lagging cover fixed in place  and rivetted","2019-09-26T23:59:35","","Completed","2019-09-24T23:59:35","No","No","No","Internal"]
[null,null,null,8136,null,"45_16/12/2019 4:16:29 PM","2019-09-20T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Following noted in 12.06.123.00.01 - Tool box meeting filed in engine room section for LFI/LET/ SAFETY FLASH etc - not filled up for entire month of september & August verification & updating in PMS after completion of JOB section not filled. ","Documentation","Cert. & Docu.","Human Error","5.1","Very High","",""," All the columns filled up ","2019-09-28T23:59:35","","Completed","2019-09-22T23:59:35","No","No","No","Internal"]
[null,null,null,8137,null,"45_16/12/2019 4:07:29 PM","2019-09-20T23:59:35","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Minor leakage  observed from NO.i&2 pilot pressure gauge connection for steering gear","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Leak rectified by tightening the connections","2019-09-25T23:59:35","","Completed","2019-09-23T23:59:35","No","No","No","Internal"]
[null,null,null,8138,null,"45_16/12/2019 4:02:11 PM","2019-09-20T23:59:35","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","NO.1/2 Boiler circulating pump gauges are incorrect scale","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.19","Very High","","","Boiler water circulating pump suction pressurte equal to the boiler drum pressure, No 1 pump prssure gauges working good, #2 pump pressure gauge renewewd.","2019-09-21T23:59:35","","Completed","2019-09-21T23:59:35","No","No","No","Internal"]
[null,null,null,8139,null,"45_16/12/2019 2:23:29 PM","2019-09-20T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Securing nut for ladder to Main COPT CSW pump observed to be loose","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.15","Low","","","Securing nut tightned","2019-09-25T23:59:35","","Completed","2019-09-20T23:59:35","No","No","No","Internal"]
[null,null,null,8140,null,"45_16/12/2019 2:48:04 PM","2019-09-20T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","AE 1  Fuel oil drain line lagging missing","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.19","Very High","","","Lagging made on drain line","2019-09-24T23:59:35","","Completed","2019-09-21T23:59:35","No","No","No","Internal"]
[null,null,null,8141,null,"45_16/12/2019 2:37:33 PM","2019-09-20T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","No.2  FWG  ejector pump gland leaking from mechanical seal","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","No gland leak, only come condensate water on top of the casing. it has been cleaned and painted.","2019-09-23T23:59:35","","Completed","2019-09-23T23:59:35","No","No","No","Internal"]
[null,null,null,8142,null,"45_16/12/2019 3:01:55 PM","2019-09-20T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","M.E NO.6 Unit jacket cooling water valve having tell tale sign of minor SW leakage","Main Engine ,E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","It is not SW , JCW FW line , no leaks observed, old salt deposits removed and painted.","2019-09-25T23:59:35","","Completed","2019-09-23T23:59:35","No","No","No","Internal"]
[null,null,null,8143,null,"45_16/12/2019 3:05:01 PM","2019-09-20T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","M.E Auto back wash filter change over valve leaking from gland","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.19","Very High","","","Changing over cock , shaft seals, aond o-rings renewed. Leak rectified.","2019-10-31T23:59:35","","Completed","2019-09-23T23:59:35","No","No","No","Internal"]
[null,null,null,8144,null,"45_16/12/2019 3:08:09 PM","2019-09-20T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","NO.1 ME F.O circulating pump pressure gauge connection having minor leake","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.19","Very High","","","Leak mark cleaned and painted.","2019-09-24T23:59:35","","Completed","2019-09-23T23:59:35","No","No","No","Internal"]
[null,null,null,8145,null,"45_16/12/2019 3:11:38 PM","2019-09-20T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","NO.2 HFO Purifier leakage vent line valve having tell tale signs","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.19","Very High","","","Purifier heater Old oil stain cleaned and painted","2019-09-25T23:59:35","","Completed","2019-09-22T23:59:35","No","No","No","Internal"]
[null,null,null,8146,null,"45_16/12/2019 3:14:13 PM","2019-09-20T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","NO.2 Purifier feed 3 way valve having minor leakage sign","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.19","Very High","","","3-Way valve gland tightened & cleaned","2019-09-21T23:59:35","","Completed","2019-09-23T23:59:35","No","No","No","Internal"]
[null,null,null,8147,null,"45_16/12/2019 3:17:03 PM","2019-09-20T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","AUX BOILER NO.2 Fuel oil heater temp thermometer unlegible","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.19","Very High","","","New thermometer fitted","2019-09-26T23:59:35","","Completed","2019-09-22T23:59:35","No","No","No","Internal"]
[null,null,null,8149,null,"45_16/12/2019 3:23:47 PM","2019-09-20T23:59:35","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Port side engine room store stowage rack dont having and stopper bars","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Stopper bars fabricated and fixed","2019-10-30T23:59:35","","Completed","2019-09-20T23:59:35","No","No","No","Internal"]
[null,null,null,8150,null,"45_16/12/2019 3:36:27 PM","2019-09-20T23:59:35","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Recommended to  fit safety gaurd for both hydrophore distill water pump","Miscellaneous,E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.28","Low","","","Gaurds fabricated and fitted.","2019-09-27T23:59:35","","Completed","2019-09-25T23:59:35","No","No","No","Internal"]
[null,null,null,8151,null,"45_16/12/2019 3:27:18 PM","2019-09-20T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","1 no.s chain block in engine room store observed to be with out safety locking plates on hook","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.28","Low","","","Safety locking plate fitted on chain block","2019-09-30T23:59:35","","Completed","2019-09-27T23:59:35","No","No","No","Internal"]
[null,null,null,8152,null,"45_16/12/2019 3:30:09 PM","2019-09-20T23:59:35","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Portable ladders in engine room to be inspected and ID marked","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.28","Low","","","Inspection done and  ID tags fitted","2019-09-30T23:59:35","","Completed","2019-09-26T23:59:35","No","No","No","Internal"]
[null,null,null,8153,null,"45_16/12/2019 3:42:04 PM","2019-09-20T23:59:35","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Door packing for steering gear room entrance door(A 60) requires to be replaced at the bottom area","Miscellaneous,E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.28","Low","","","Door packing replaced ","2019-09-24T23:59:35","","Completed","2019-09-22T23:59:35","No","No","No","Internal"]
[null,null,null,8154,null,"45_16/12/2019 3:45:39 PM","2019-09-20T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Inspection resords and ID tag to be fitted on block and shackle for emergency escape rescue arrangement","Miscellaneous,E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Behaviour Based","10.28","Low","","","ID tags fitted","2019-09-28T23:59:35","","Completed","2019-09-26T23:59:35","No","No","No","Internal"]
[null,null,null,8155,null,"45_16/12/2019 3:48:40 PM","2019-09-20T23:59:35","Critical Equipment","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Gas mask outside of chemical locker to be removed as it does not have expiry date on the catridge","LSA / FFA","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Catridge type mask replaced with disposible masks  ","2019-09-27T23:59:35","","Completed","2019-09-22T23:59:35","No","No","No","Internal"]
[null,null,null,8156,null,"45_16/12/2019 3:52:06 PM","2019-09-20T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Gasket for steam atomising line for NO.1 boiler having minor leak","E/R - Boiler,E/R - Pipes/ valves & fittings","","Equipment Related","10.19","Very High","","","Leak rectified by renewing gasket","2019-09-30T23:59:35","","Completed","2019-09-25T23:59:35","No","No","No","Internal"]
[null,null,null,8157,null,"45_16/12/2019 3:55:49 PM","2019-09-20T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Date of oxygen analyzer calibration prior discharge operation to be update","Inert Gas","Eng. / Strg. Comp.","Equipment Related","8.26","High","","","Date of oxygen analyzer calibration updated ","2019-09-24T23:59:35","","Completed","2019-09-20T23:59:35","No","No","No","Internal"]
[null,null,null,8158,null,"45_16/12/2019 3:59:22 PM","2019-09-20T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Emergency stop IMO symbol to be pasted near Aux engine emergency stop buttons","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.28","Low","","","Emergency stop IMO symbols pasted","2019-09-23T23:59:35","","Completed","2019-09-21T23:59:35","No","No","No","Internal"]
[null,null,null,8159,null,"45_16/12/2019 4:12:16 PM","2019-09-20T23:59:35","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","UMS alarm for NO.2 GE F.O pressure on 13th sept 2019-0021 hrs lt not recorded in rest hour records for duty engineer","Documentation","Cert. & Docu.","Equipment Related","3.3","High","",""," Entry corrected","2019-09-27T23:59:35","","Completed","2019-09-20T23:59:35","No","No","No","Internal"]
[null,null,null,8160,null,"45_18/12/2019 10:24:02 AM","2019-09-20T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Salt deposit observed on bulb of forward liferaft embarkation light and light not working","Elect. Mach. & Equip.","","Equipment Related","11.11","Very High","","","Replaced light, cleaned lamp, applied silicon sealant, gasket","2019-10-20T23:59:35","","Completed","2019-09-22T23:59:35","No","No","No","Internal"]
[null,null,null,8161,null,"45_18/12/2019 10:31:07 AM","2019-09-20T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Water inside light fixture for WIND ALARM on bridge front.","Elect. Mach. & Equip.","General Appearance","Equipment Related","11.1","High","","","Cleaned the fixtures used silicone and applied gaskets.","2019-09-25T23:59:35","","Completed","2019-09-22T23:59:35","No","No","No","Internal"]
[null,null,null,8126,null,"45_16/12/2019 11:04:58 AM","2019-09-21T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Recommend to have close up inspection of Teflon rollers of both gangways as suspect deterioration in condition. Just by rubbing hands on the roller powder is coming out","Deck - Machinery","ISM Related","External Factors","5.47","Medium","","","Close up Inspection carried out & damage found to be only superficial.","2019-12-21T23:59:35","","Completed","2019-10-04T23:59:35","No","No","No","Internal"]
[null,null,null,6271,null,"45_Wed Jul 10 2019 22:41:37 GMT+0000 (Coordinated Universal Time)","2019-09-22T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Whistle for 1 nos SCBA set (Helicopter Equipment) not working","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.43","High","","","On receival of spare, renewed the same & function test carried out, found working satisfactory.","2019-12-31T23:59:35","SCAN 190174","Completed","2019-12-25T23:59:35","No","No","No","Internal","Will be supplied in Qingdao."]
[null,null,null,8093,null,"45_18/12/2019 3:27:43 PM","2019-09-22T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Signai light column not working, Near Boiler all lights not working, Outside Purifier room, Inside purifier room, Inside engine room workshop.","Elect. Mach. & Equip.","General Appearance","Equipment Related","11.9","Low","","","Signal light column lights renewed.Working good.","2020-02-25T23:59:35","RO SCAN 190173","Completed","2020-01-27T23:59:35","No","No","No","Internal","Item ready, will be supplied at next opportunity. Target date revised accordingly."]
[null,null,null,8096,null,"45_Sun May 12 2019 15:09:22 GMT+0000 (Coordinated Universal Time)","2019-09-22T23:59:35","Defect","Owner / Marine / Tech. Suptd.","ISPS Audit","ISPS Audit - Various different drill scenario’s\n\nrequired to be covered as per SSP-12.01 not\n\ncarried out last 1 year","Documentation","ISPS Related","Human Error","7.4","Low","","","Drills as per SSP 12.01 were carried out for the year in the month of September.\n\nAttached ISPS Drills carried out in last 1 year for reference. All joining officers must \n\nfamiliarize themselves with the company's requirement for frequency of Drills.","2019-12-21T23:59:35","","Completed","2019-10-04T23:59:35","No","No","No","Internal"]
[null,null,null,8097,null,"45_Sun May 12 2019 15:16:52 GMT+0000 (Coordinated Universal Time)","2019-09-22T23:59:35","Non Conformity","Owner / Marine / Tech. Suptd.","ISM Audit","Oil Soaked Lagging noted around\n\nF.O Transfer pump suction filter","E/R - Pipes/ valves & fittings","General Appearance","Human Error","10.19","Very High","","","Renewed oil soaked lagging. While cleaning filter  filter casing should be drained of oil prior removing filter element. Oil soaked lagging if found to be renewed immediately.","2019-12-21T23:59:35","","Completed","2019-10-09T23:59:35","No","No","No","Internal"]
[null,null,null,8098,null,"45_Sun May 12 2019 15:27:31 GMT+0000 (Coordinated Universal Time)","2019-09-22T23:59:35","Non Conformity","Owner / Marine / Tech. Suptd.","ISM Audit","Vessel is equipped with Unitor 15H & Fangzhan TH/15 EEBD's. However donning\n\n& maintenance instructions were not included for Fangzhan TH/15 inside Fire training manual and Fire & safety Operational booklet","Documentation","Safety / LSA / FFA","Human Error","5.34","Low","","","Donning Instructions for Fangzhan TH/15 EEBD were inserted in Fire training Manual & safety Operational booklet. Officer made aware of the requirement for inserting the maker's instructions in case of any changes in LSA/FFA equipments. Training imparted to the responsible officer for the informations that should be available inside Fire training Manual & safety Operational booklet\n\nSame to be monitored & verified in future Fire & safety Operational booklet by Master.","2019-12-21T23:59:35","","Completed","2019-10-04T23:59:35","No","No","No","Internal"]
[null,null,null,8099,null,"45_Sun May 12 2019 15:35:31 GMT+0000 (Coordinated Universal Time)","2019-09-22T23:59:35","Defect","Owner / Marine / Tech. Suptd.","ISM Audit","Rubber Insulation Mat was missing in front of Hydraulic starter panel (440v) & L-7 panel (440v) inside forward bosun store.","Elect. Mach. & Equip.","ISM Related","Human Error","10.24","Low","","","All Crew were briefed about the importance of rubber insulation mats near a switch board for their own safety & if any place the mat is found missing this should be brought to notice of \n\nETO immediately. ETO will include in his weekly wet rounds the position of  rubber insulation mats at each electrical panel to avoid such incidence in future.","2019-12-21T23:59:35","","Completed","2019-10-11T23:59:35","No","No","No","Internal"]
[null,null,null,8100,null,"45_Sun May 12 2019 15:53:11 GMT+0000 (Coordinated Universal Time)","2019-09-22T23:59:35","Defect","Owner / Marine / Tech. Suptd.","ISM Audit","Securing shackle for forward life\n\nraft embarkation ladder was observed to be\n\nheavily rusted and difficult to open","LSA / FFA","Safety / LSA / FFA","Human Error","5.27","Medium","","","Securing shackle for forward life\n\nraft embarkation ladder was freed & greased immediately. Company Maintenance schedule to be followed and implemented as per company Requirement  & Industry Standard.","2019-12-22T23:59:35","","Completed","2019-10-10T23:59:35","No","No","No","Internal"]
[null,null,null,8101,null,"45_Sun May 12 2019 16:03:31 GMT+0000 (Coordinated Universal Time)","2019-09-22T23:59:35","Defect","Owner / Marine / Tech. Suptd.","ISM Audit","Paint Drums in paint locker were\n\nobserved to be stored in double stack above the stopper bar.","Miscellaneous","","Human Error","5.46","Medium","","","All crew members were briefed about hazards involved in stowing paint drums in double stack, they were informed about company procedure clearly stating such stowage is not allowed and single stack stowage should be strictly followed in future.","2019-12-21T23:59:35","","Completed","2019-10-04T23:59:35","No","No","No","Internal"]
[null,null,null,8102,null,"45_Sun May 12 2019 16:15:18 GMT+0000 (Coordinated Universal Time)","2019-09-22T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Nav Audit / Verification","Value for Correction for Sea / Swell / Wave response allowance in section-3 - controlling depth calculation in form 12.01.14.021.00 - UKC calculation form were observed to be used as -0.10 Mtrs for all previous ports rather than basis actual anticipated weather.","Documentation","Navigation","Human Error","4.5","Very High","","","Training carried out by Supt for correct procedure to apply correction value. Same will be monitored & verified in future passage plan by Master.\n\n","2019-12-21T23:59:35","","Completed","2019-10-02T23:59:35","No","No","No","Internal"]
[null,null,null,8103,null,"45_Sun May 12 2019 16:20:32 GMT+0000 (Coordinated Universal Time)","2019-09-22T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Mooring Audit","Gear engaging lever disengaging on port side mooring winch number 1&2 due to excessive play.","Deck - Mooring Machinery","Mooring","Human Error","9.14","Medium","","","The locking arrangement for Winch 1 & 2 were aligned and checked for proper operation.","2019-12-20T23:59:35","","Completed","2019-10-10T23:59:35","No","No","No","Internal"]
[null,null,null,8104,null,"45_Sun May 12 2019 16:09:01 GMT+0000 (Coordinated Universal Time)","2019-09-22T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ME Auto back wash filter heating\n\nsteam valve leaking","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Valve gland packing renewed and leakage rectified. Regular checking of leakage and  preventive maintenance to be done in time. ","2019-12-21T23:59:35","","Completed","2019-10-09T23:59:35","No","No","No","Internal"]
[null,null,null,8106,null,"45_15/12/2019 7:06:05 PM","2019-09-22T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Bottom rubber packing for paint locker natural vent missing","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","Human Error","11.7","High","","","Bottom Rubber packing for paint locker was replaced.","2019-09-25T23:59:35","","Completed","2019-12-21T23:59:35","No","No","No","Internal"]
[null,null,null,8107,null,"45_15/12/2019 7:14:31 PM","2019-09-22T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Drums in paint locker stowed in double layer above stopper bar","Accommodation ,Miscellaneous","Cargo / Ballast Systems","Human Error","5.11","Low","","","Drums were removed,secured and stowed properly.All crew members were briefed about hazards involved in stowing paint drums in double stack, they were informed about company procedure clearly stating such stowage is not allowed and single stack stowage should be strictly followed in future.","2019-12-21T23:59:35","","Completed","2019-10-04T23:59:35","No","No","No","Internal"]
[null,null,null,8108,null,"45_15/12/2019 7:47:45 PM","2019-09-22T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Brake indicators of mooring winches observed to be not aligned when brake applied","Deck - Machinery","Mooring","Human Error","9.7","Medium","","","Brake indicators for mooring winches were alligned after tightening the brakes for all the winches","2019-12-21T23:59:35","","Completed","2019-09-28T23:59:35","No","No","No","Internal"]
[null,null,null,8109,null,"45_15/12/2019 7:53:51 PM","2019-09-22T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Key for ‘Emergency generator room Co2 release’ cabinet to be stored at common location","LSA / FFA","Safety / LSA / FFA","Human Error","5.4","High","","","Key for Emergency Generator Room CO2 Release Cabinet was stored in Ships Office and all Crew were made aware about it.","2019-12-21T23:59:35","","Completed","2019-09-25T23:59:35","No","No","No","Internal"]
[null,null,null,8110,null,"45_15/12/2019 7:57:16 PM","2019-09-22T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Inspection records and ID tags for web slings","Miscellaneous","Mooring","Human Error","10.28","Low","","","Inspection Records and ID Tags for Web Slings were made and filed as required.","2019-12-21T23:59:35","","Completed","2019-09-30T23:59:35","No","No","No","Internal"]
[null,null,null,8111,null,"45_Sun Dec 15 2019 20:04:52 GMT+0000 (Coordinated Universal Time)","2019-09-22T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Forward bosun store Bilge overboard discharge to be sealed","Deck - Pipe / Fittings","Cargo / Ballast Systems","Human Error","6.15","High","","","Forward Bosun store Bilge Overboard Discharge were sealed and same inserted in Environmental Seal Log","2019-12-21T23:59:35","","Completed","2019-09-26T23:59:35","No","No","No","Internal"]
[null,null,null,8112,null,"45_Sun Dec 15 2019 20:08:40 GMT+0000 (Coordinated Universal Time)","2019-09-22T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Dresser for IG line on top of 2C COT having minor leakage  ","Inert Gas","Cargo / Ballast Systems","External Factors","8.23","Medium","","","Dresser for IG line on top of 2C COT was tightened and leak stopped.","2019-12-21T23:59:35","","Completed","2019-09-26T23:59:35","No","No","No","Internal"]
[null,null,null,8113,null,"45_Sun Dec 15 2019 20:43:45 GMT+0000 (Coordinated Universal Time)","2019-09-22T23:59:35","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Recommend to fabricate quick release arrangement for embarkation ladder cover or keep a knife standby to remove the cover in minimum time.","LSA / FFA","Safety / LSA / FFA","Human Error","5.47","Medium","","","Knife has been kept standby to remove the embarkation ladder cover in minimum time.","2019-12-21T23:59:35","","Completed","2019-09-30T23:59:35","No","No","No","Internal"]
[null,null,null,178,null,"45_Wed Jul 10 2019 06:33:22 GMT+0000","2019-09-22T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","145 ltr foam fire extinguisher on boiler platform having superficial cracks on the flexible hose","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.42","Medium","","","new extinguisher rcvd. Put in use.","2019-12-31T23:59:35","SCAN 190174","Completed","2019-12-25T23:59:35","No","No","No","Internal","Will be supplied in Qingdao."]
[null,null,null,8114,null,"45_Sun Dec 15 2019 20:45:49 GMT+0000 (Coordinated Universal Time)","2019-09-22T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Shackle for forward embarkation ladder heavily corroded","LSA / FFA","Safety / LSA / FFA","Human Error","5.47","Medium","","","Shackle for forward embarkation ladder was replaced.","2019-12-21T23:59:35","","Completed","2019-09-25T23:59:35","No","No","No","Internal"]
[null,null,null,8115,null,"45_Sun Dec 15 2019 20:48:58 GMT+0000 (Coordinated Universal Time)","2019-09-22T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Port Side Lifeboat Side glass has become translucent","LSA / FFA","Safety / LSA / FFA","External Factors,Human Error","5.29","High","","","Port Side Lifeboat Side Glass has been replaced.","2019-12-21T23:59:35","","Completed","2019-10-20T23:59:35","No","No","No","Internal"]
[null,null,null,8116,null,"45_16/12/2019 9:22:46 AM","2019-09-22T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Bottom wire for safe access to tanker bow walkway missing ","Miscellaneous","General Appearance","Human Error","12.9","High","","","Walkway Wires were checked and inserted were required","2019-12-21T23:59:35","","Completed","2019-09-23T23:59:35","No","No","No","Internal"]
[null,null,null,8117,null,"45_16/12/2019 9:28:47 AM","2019-09-22T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Safety latch for hook of 1 nos chain block is missing & fitted on outside of the hooks ","Miscellaneous","Mooring","Human Error","10.28","Low","","","Safety latches for all chain blocks were checked and renewed as required .","2019-12-21T23:59:35","","Completed","2019-09-30T23:59:35","No","No","No","Internal"]
[null,null,null,8118,null,"45_16/12/2019 9:52:18 AM","2019-09-22T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Few aluminum ladder on deck observed to be without bottom rubber packing","Miscellaneous","General Appearance","Human Error","12.9","High","","","All Aluminium Ladders were checked for their bottom rubber packing and were renewed where required.","2019-12-21T23:59:35","","Completed","2019-10-14T23:59:35","No","No","No","Internal"]
[null,null,null,8119,null,"45_16/12/2019 9:58:26 AM","2019-09-22T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","1 nos dresser coupling on 5C COT having minor leakage","Deck - Pipe / Fittings","Cargo / Ballast Systems","External Factors","8.15","High","","","Dresser coupling was tightened as required , leak was rectified","2019-12-21T23:59:35","","Completed","2019-09-23T23:59:35","No","No","No","Internal"]
[null,null,null,8120,null,"45_16/12/2019 10:00:34 AM","2019-09-22T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","12.06.015.001 – PPE guide in use on board is old version","Documentation","Cert. & Docu.","Human Error","5.5","Low","","","PPE guide was replaced with latest version","2019-12-21T23:59:35","","Completed","2019-09-23T23:59:35","No","No","No","Internal"]
[null,null,null,8121,null,"45_16/12/2019 10:05:05 AM","2019-09-22T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Drug & Alcohol policy pasted in alleyways and common places to be updated with the latest version","Documentation","Cert. & Docu.","Human Error","3.8","Very High","","","Drug & Alcohol policy pasted in alleyways and common places was updated ","2019-12-21T23:59:35","","Completed","2019-09-24T23:59:35","No","No","No","Internal"]
[null,null,null,8122,null,"45_16/12/2019 10:16:14 AM","2019-09-22T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Vessel is provided with Unitor 15H & FANGZHAN TH/15-1 EEBD’s. However donning & maintenance instructions are missing from Fire training Manual and fire & safety operational booklet","LSA / FFA","Safety / LSA / FFA","Human Error","5.15","Medium","","","Donning Instructions for Fangzhan TH/15 EEBD were inserted in Fire training Manual & safety Operational booklet. Officer made aware of the requirement for inserting the maker's instructions in case of any changes in LSA/FFA equipments.","2019-12-21T23:59:35","","Completed","2019-10-04T23:59:35","No","No","No","Internal"]
[null,null,null,8123,null,"45_16/12/2019 10:27:26 AM","2019-09-22T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Securing strap of spare BA set bottle in foam room broken.","LSA / FFA","Safety / LSA / FFA","Human Error","8.65","Low","","","Securing strap replaced & BA set Bottles secured properly.","2019-12-21T23:59:35","","Completed","2019-09-23T23:59:35","No","No","No","Internal"]
[null,null,null,8124,null,"45_16/12/2019 10:39:52 AM","2019-09-22T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Seals for 2 spare fire extinguishers missing","LSA / FFA","Safety / LSA / FFA","Human Error","5.42","Medium","","","Seals for Extinguishers were placed back fot the 2 spare fire Extinguishers.","2019-12-21T23:59:35","","Completed","2019-09-24T23:59:35","No","No","No","Internal"]
[null,null,null,8125,null,"45_16/12/2019 10:51:05 AM","2019-09-22T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Close Indicator for Fire main isolation valve to upper deck not matching with close indicator when fully closed","LSA / FFA","Safety / LSA / FFA","Equipment Related","11.4","Very High","","","Close Indicator for Fire main isolation valve to upper deck was replaced & matched when fully closed.","2019-12-21T23:59:35","","Completed","2019-09-24T23:59:35","No","No","No","Internal"]
[null,null,null,8127,null,"45_16/12/2019 11:11:43 AM","2019-09-22T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Gear engaging lever taper has worn out for port side mooring winch number 1 & 2. Recommend to inspect all","Deck - Machinery","Mooring","External Factors","9.15","Medium","","","The locking arrangement for Winch 1 & 2 were aligned and checked for proper operation.","2019-12-21T23:59:35","","Completed","2019-10-10T23:59:35","No","No","No","Internal"]
[null,null,null,8128,null,"45_16/12/2019 11:15:43 AM","2019-09-22T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Gap in rubber packing of port side upper deck watertight door when fully closed","Accommodation","Structural Condn. / WT integrity ","External Factors","11.6","Medium","","","Rubber packing of Port side upper deck watertight door was replaced and no gaps found.","2019-12-21T23:59:35","","Completed","2019-10-10T23:59:35","No","No","No","Internal"]
[null,null,null,8129,null,"45_16/12/2019 11:21:51 AM","2019-09-22T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","No-3 foam monitor valve hard to open","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.35","Medium","","","No-3 Foam monitor valve was freed up , greasing carried out and found to be free","2019-11-21T23:59:35","","Completed","2019-10-03T23:59:35","No","No","No","Internal"]
[null,null,null,8130,null,"45_16/12/2019 11:41:35 AM","2019-09-22T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Engine room fire isolation valve in foam room has shaft slightly bent making it hard to close the valve.","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.35","Medium","","","On Detailed inspection it was found that the tightness was due to the dryness of the gland, shaft observed to be in prestine condition, the bend was on the indicator of the valve which has been rectified.Required maintainance carried out on  the gland & valve, found to be closing smoothly.","2019-12-21T23:59:35","","Completed","2019-10-05T23:59:35","No","No","No","Internal"]
[null,null,null,6272,null,"45_Wed Jul 10 2019 22:47:16 GMT+0000 (Coordinated Universal Time)","2019-10-01T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","Engine room crane traverse PORT- STBD motor not working","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.28","Low","","","Traverse motor renewed with spare recieved. Working satisfactory","2019-12-16T23:59:35","SCAN190175","Completed","2019-12-15T23:59:35","No","No","No","Internal","Spares being supplied in Qingdao."]
[null,null,null,8094,null,"45_Sun May 12 2019 14:58:55 GMT+0000 (Coordinated Universal Time)","2019-10-07T23:59:35","Defect","Ship Staff","Nav Audit / Verification","In Master-Pilot Information Exchange, while approaching Singapore anchorage with Pilot onboard the number of shackles  and which anchor planned for use at anchorage was not mentioned.","Navigation - Others","Navigation","Human Error","4.3","Medium","","","Responsible officer was briefed on the entry  regarding the number of shackles & which anchor to be used shall be mentioned in the Master-Pilot Information Exchange when vessel is proceeding to anchorage under pilotage. Master carried out briefing of Navigational watchkeepers and appraised them regarding mandatory entries to be made in Master Pilot Information exchange.","2020-01-06T23:59:35","","Completed","2019-10-23T23:59:35","No","No","No","Internal"]
[null,null,null,8095,null,"45_Sun May 12 2019 15:03:04 GMT+0000 (Coordinated Universal Time)","2019-10-07T23:59:35","Defect","Ship Staff","Nav Audit / Verification","Performance of the echo sounder was not tested on all ranges and scales to verify recordings against depths shown on the chart.","Navigation - Echo Sounder / Speed Log","Navigation","Human Error","4.7","High","","","Responsible Officer was briefed by  Master on the requirement for testing the Performance of the echo sounder on all ranges and scales to verify recordings against depths shown on the chart. Master carried out training of all Navigating officers regarding all Navigational equipment check procedures as required by company sms.","2020-01-06T23:59:35","","Completed","2019-10-23T23:59:35","No","No","No","Internal"]
[null,null,null,6269,null,"45_Sat Nov 02 2019 09:53:17 GMT+0000 (Coordinated Universal Time)","2019-10-24T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Observed leakage through fuel back wash  filter change over cock shaft seal while Auxiliary Engines change over to LSMGO","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.1","Medium","","","O-rings/seal rings renwed and leakage rectified.","2019-10-25T23:59:35","","Completed","2019-10-24T23:59:35","No","No","No","Internal"]
[null,null,null,6274,null,"45_Mon Feb 11 2019 12:22:13 GMT+0000 (Coordinated Universal Time)","2019-10-24T23:59:35","Defect","Ship Staff","Ship Staff Insp.","High Wind strobe light infront of Bridge found wasted. Buzzer for the same in CCR not operational.","Elect. Mach. & Equip.","Cargo / Ballast Systems","Equipment Related","4.5","Very High","","","Strobe light renewed. Buzzer in CCR also renewed.","2020-02-24T23:59:35","SCAN190181","Completed","2020-01-25T23:59:35","No","No","No","Internal","Spare will be ready by 6th Jan. TArget date revised accordingly."]
[null,null,null,6270,null,"45_15/11/2019 3:24:49 AM","2019-11-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Fresh water generator ejector pump #1 discharge valve SW leaking from the gland.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.31","Very High","","","Complete valve bonnet renewed as parts wasted.","2019-11-05T23:59:35","","Completed","2019-11-02T23:59:35","No","No","No","Internal"]
[null,null,null,6275,null,"45_15/11/2019 3:33:56 AM","2019-11-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","FWG Ejector pump #1 Mechanical seal leaking","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.31","Very High","","","Pump has been overhauled , Mechanical seal renewed.","2019-11-05T23:59:35","","Completed","2019-11-02T23:59:35","No","No","No","Internal"]
[null,null,null,6276,null,"45_15/11/2019 4:50:40 AM","2019-11-09T23:59:35","Defect","Ship Staff","Ship Staff Insp.","During Saturday safety routine observed Portside lifeboat engine was not starting on No.1 battery","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.27","Medium","","","Battery renewed with new spare.","2019-11-10T23:59:35","","Completed","2019-11-10T23:59:35","No","No","No","Internal"]
[null,null,null,6273,null,"45_16/11/2019 2:48:08 PM","2019-11-14T23:59:35","Other","Ship Staff","Ship Staff Insp.","Anemometer was found damaged in Heavy weather","Navigation - Others","Navigation","External Factors","4.2","Medium","","","Vessel has installed spare anemometer available onboard. Requisitons for spare anemometer has been raised in PAL.","2019-11-30T23:59:35","SCAN190193 ANEMOMETER TRANSMITTER 3 CUP TYPE","Completed","2019-11-19T23:59:35","No","No","No","Internal","Understand , job completed."]
[null,null,null,7058,null,"45_Sun Dec 01 2019 11:50:07 GMT+0000 (Coordinated Universal Time)","2019-11-17T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","HFO purifier #2 breakdown due to bearing failure. Bearing & Spindle found damaged","E/R - Purifier","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Service technician attended for the job. Renewed all necessary parts. working satisfactory.","2019-12-15T23:59:35","","Completed","2019-12-14T23:59:35","No","No","No","Internal","Spares will be supplied in China, Qingdao."]
[null,null,null,16129,null,"45_11/12/2020 10:42:26 PM","2019-11-19T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ECGS deck house exit door handle to stencil O/C , also provide baton.","Miscellaneous","General Appearance","Human Error","","","","","ECGS deck house exit door handle stenciled  O/C , also provided baton.","2020-11-29T23:59:35","","Completed","2020-11-25T23:59:35","No","No","No","Internal"]
[null,null,null,8105,null,"45_Mon Aug 12 2019 13:48:56 GMT+0000 (Coordinated Universal Time)","2019-11-19T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Bunker Transfer Plan / Checklist 12.04.08.011.01 Section 7 - Monitoring of H2S/Benzene Vapors : Benzene reading measured by detector tubes shall be mentioned < Min value that can be measured by the specific tube. For example by Gastec tubes Min measurable value is 0.05 ppm, hence in that case benzene shall be mention <0.05 ppm (if no discoloration observed)\n\nUnderstand vessel has kept the Gas tubes as evidence of monitoring. \n\n","Documentation","ISM Related","Human Error","5.23","Very High","","","Corrective Action : Vessel is having Gastec tubes onboard with minimum value of  0.1 ppm. Corrected benzene measured value as <0.1ppm in the checklist. Scanned copy attached.\n\nPreventive action : Responsible officer engineer has been briefed regarding use of Gastec tubes and entries to be made in Checklists.","2020-02-28T23:59:35","","Completed","2019-11-30T23:59:35","No","No","No","Internal"]
[null,null,null,7060,null,"45_Sat Jan 12 2019 17:36:33 GMT+0000 (Coordinated Universal Time)","2019-11-22T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Pump room blower(Port)found with excessive vibration during running","Deck - Machinery","Cargo / Ballast Systems","Equipment Related","5.18","High","","","Blower inspected and found spider coupling damaged . Same renewed.Working satisfactory.","2019-11-27T23:59:35","","Completed","2019-11-25T23:59:35","No","No","No","Internal"]
[null,null,null,7059,null,"45_Sun Dec 01 2019 11:54:32 GMT+0000 (Coordinated Universal Time)","2019-11-29T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","HFO purifier #1 breakdown due to bearing failure, Top bearing , spindle found damaged","E/R - Purifier","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","ALFALAVAL service technician attended the job, purifier overhauled with new spare parts received. Tested and working satisfactory.","2019-12-31T23:59:35","SCAN 190178, SCAN190214","Completed","2019-12-24T23:59:35","No","No","No","Internal","Spares and service is arranged for Singapore. Hence target date revised."]
[null,null,null,9405,null,"45_02/01/2020 11:01:52 AM","2019-12-02T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Ship Staff Insp.","Main Engine FO viscotherm found not working","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.1","Medium","","","Attended during docking and presently working fine.","2021-01-30T23:59:35","SCAN 200004","Completed","2020-11-30T23:59:35","No","No","No","Internal",""]
[null,null,null,174,null,"45_Wed Jul 10 2019 02:04:42 GMT+0000","2019-12-07T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","LT cooling line to AEs, running below AE Gen platform – soft patch and leaking","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","To repair or renew the pipe section during next Dry Dock. Job shifted to refman.","2020-02-20T23:59:35","","Completed","2020-07-20T23:59:35","Yes","No","No","Internal","Job to be attended during docking."]
[null,null,null,9406,null,"45_02/01/2020 11:11:34 AM","2019-12-12T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Ship Staff Insp.","No.1. Boiler pilot burner actuator erratic .","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Actuator renewed with spare received.","2020-02-28T23:59:35","SCAN190226","Completed","2020-01-24T23:59:35","No","No","No","Internal","Spares will be supplied this call Singapore."]
[null,null,null,9402,null,"45_31/12/2019 8:08:17 PM","2019-12-15T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","On boiler FD fan platform, areas which are near the blower duct are in very dirty condition, to clean.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","External Factors","10.29","Medium","","","Cleaned and painted","2020-02-28T23:59:35","","Completed","2020-01-02T23:59:35","No","No","No","Internal"]
[null,null,null,9403,null,"45_31/12/2019 8:04:28 PM","2019-12-15T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Electrical store are on the expansion tank platform to arrange.","Miscellaneous","Eng. / Strg. Comp.","Knowledge Based","10.29","Medium","","","Eklectrical stores arranged ","2020-02-22T23:59:35","","Completed","2020-02-10T23:59:35","No","No","No","Internal"]
[null,null,null,9407,null,"45_03/01/2020 2:52:58 PM","2019-12-15T23:59:35","Observation,Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Bridge air con base plate is completely corroded. To repair.","Miscellaneous","Structural Condn. / WT integrity ","Human Error,Inappropriate Procedure,Knowledge Based","11.8","Low","","","Temporary repairs made, added to Refman for DD repairs","2020-03-15T23:59:35","","Completed","2020-01-02T23:59:35","No","No","No","Internal"]
[null,null,null,9408,null,"45_03/01/2020 3:02:12 PM","2019-12-15T23:59:35","Defect,Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Various bunker tanks man hole door handle is frozen in lifted condition and posing as hazard. TO free up.","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","External Factors,Human Error","11.8","Low","","","Hydroblasted & painted. Verified free movement of handles.","2020-01-30T23:59:35","","Completed","2020-01-15T23:59:35","No","No","No","Internal"]
[null,null,null,9409,null,"45_03/01/2020 3:06:11 PM","2019-12-15T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","VDR junction box base plate on monkey island is mildly corroded. To renew.","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","External Factors,Human Error,Knowledge Based","11.8","Low","","","VDR junction box base plate rust removed and painted.It will be removed during new VDR installation planned.","2020-02-20T23:59:35","","Completed","2020-03-03T23:59:35","No","No","No","Internal"]
[null,null,null,9410,null,"45_31/12/2019 8:12:18 PM","2019-12-15T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Dishwasher is not operational, to order parts.","Accommodation ","Eng. / Strg. Comp.","Equipment Related","11.16","Low","","","New diswasher installed. Working satisfactorily","2020-09-30T23:59:35","SCAN 200005","Completed","2020-10-31T23:59:35","Yes","No","No","Internal","Target date revised due to spares lead time. Same will be supplied during docking"]
[null,null,null,9411,null,"45_31/12/2019 8:17:40 PM","2019-12-15T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Door lock arrangement from funnel to E/R blower platform needs to be repaired.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Plate fabricated and door lock arrangement repaired.","2020-03-28T23:59:35","","Completed","2020-03-04T23:59:35","No","No","No","Internal"]
[null,null,null,9412,null,"45_01/01/2020 6:53:27 PM","2019-12-15T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ME Running hour meter not working. To order.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.37","Medium","","","trouble shooting done presently working good. RO raised for new spare","2020-02-28T23:59:35","","Completed","2019-12-31T23:59:35","No","No","No","Internal"]
[null,null,null,9413,null,"45_03/01/2020 3:10:14 PM","2019-12-15T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Sludge storage tank paint has peeled off. To paint.","Deck - Pipe / Fittings","General Appearance","External Factors,Human Error,Knowledge Based","11.3","Medium","","","Surface preparation carried out & painted.","2020-03-30T23:59:35","","Completed","2020-03-20T23:59:35","No","No","No","Internal"]
[null,null,null,9414,null,"45_01/01/2020 6:58:23 PM","2019-12-15T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","In workshop there is no stopper for pipe storage area. To fabricate.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Knowledge Based","10.28","Low","","","Stopper fabricated and fitted","2020-01-25T23:59:35","","Completed","2020-01-15T23:59:35","No","No","No","Internal"]
[null,null,null,9415,null,"45_31/12/2019 7:58:47 PM","2019-12-15T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Both Air bottle auto drain is leaking and hence kept shut. To overhaul.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Auto drain sOverhauled and kept open","2019-12-30T23:59:35","","Completed","2019-12-20T23:59:35","No","No","No","Internal"]
[null,null,null,9416,null,"45_31/12/2019 8:02:20 PM","2019-12-15T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Ship Staff Insp.","Air compressor, air bottles and air con compressor / motor to soap wash. Found in dirty condition.","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related","","","","","Soap washed & Cleaned","2020-01-15T23:59:35","","Completed","2019-12-19T23:59:35","No","No","No","Internal"]
[null,null,null,9417,null,"45_31/12/2019 8:20:18 PM","2019-12-15T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Main power light in CO2 room for power change over box not working.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.37","Medium","","","Indication Lamp Renewed","2019-12-22T23:59:35","","Completed","2019-12-19T23:59:35","No","No","No","Internal"]
[null,null,null,9420,null,"45_03/01/2020 2:48:19 PM","2019-12-15T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","BA compressor is fixed in place with rope. TO make permanent arrangement.","LSA / FFA","Safety / LSA / FFA","External Factors,Human Error","5.11","Low","","","Permanent arrangement made.","2019-12-30T23:59:35","","Completed","2019-12-18T23:59:35","No","No","No","Internal"]
[null,null,null,9421,null,"45_03/01/2020 3:14:15 PM","2019-12-15T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","No 2 Outer HFO tank save all is not stencilled for its capacity. ","Deck - Pipe / Fittings","General Appearance","External Factors,Human Error,Knowledge Based","11.8","Low","","","Capacity Stenciled","2019-12-20T23:59:35","","Completed","2019-12-18T23:59:35","No","No","No","Internal"]
[null,null,null,9422,null,"45_03/01/2020 3:16:10 PM","2019-12-15T23:59:35","Non Conformity","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Pump room weather tight door packing to renew. Light passing even when door is fully closed.","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","External Factors,Human Error","11.6","Medium","","","Packing renewed","2019-12-30T23:59:35","","Completed","2019-12-30T23:59:35","No","No","No","Internal"]
[null,null,null,9423,null,"45_03/01/2020 3:08:36 PM","2019-12-15T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Ladder outside paint locker is in very dirty condition. To clean and paint.","Deck - Pipe / Fittings","General Appearance","External Factors,Human Error,Inappropriate Procedure,Knowledge Based","11.3","Medium","","","Cleaning of ladders & steps carried out.","2019-12-30T23:59:35","","Completed","2019-12-19T23:59:35","No","No","No","Internal"]
[null,null,null,9404,null,"45_02/01/2020 9:21:59 AM","2019-12-21T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Ship Staff Insp.","During testing of emergency generator found tachometer not working.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.37","Medium","","","Tachometer  renwed. working satisfactory","2020-02-21T23:59:35","SCAN190230","Completed","2020-02-06T23:59:35","No","No","No","Internal"]
[null,null,null,9418,null,"45_02/01/2020 9:15:04 AM","2019-12-21T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Ship Staff Insp.","During saturday routines observed Emergency generator not starting on battery","Elect. Mach. & Equip.","Emgcy. Systems","Equipment Related","10.36","Very High","","","Battery renewed with spare onboard, tested working satisfactory.","2019-12-22T23:59:35","","Completed","2019-12-21T23:59:35","No","No","No","Internal"]
[null,null,null,9419,null,"45_02/01/2020 11:27:07 AM","2019-12-28T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Ship Staff Insp.","During saturday routines ER ventilation fan No.4 flap actuator found leaking and cylinder and end cover material wasted.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.18","High","","","Renewed with sapre actuator onboard. Tested working satisfactory.","2019-12-31T23:59:35","","Completed","2019-12-30T23:59:35","No","No","No","Internal"]
[null,null,null,9592,null,"45_07/01/2012 1:03:59 AM","2020-01-01T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Old supports for the name board on either sides are heavily corroded, new ones to fabricate.","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","External Factors,Inappropriate Procedure","11.8","Low","","","New supports fabricated & fitted","2020-02-01T23:59:35","","Completed","2020-01-10T23:59:35","No","No","No","Internal"]
[null,null,null,9593,null,"45_07/01/2012 1:08:45 AM","2020-01-01T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Bottom Support plate for the MFHF distribution box is wasted. New one to fabricate","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","External Factors,Human Error,Inappropriate Procedure","11.8","Low","","","New Support  fabricated 7 fitted.","2020-02-01T23:59:35","","Completed","2020-01-09T23:59:35","No","No","No","Internal"]
[null,null,null,9595,null,"45_12/01/2020 9:50:49 AM","2020-01-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","ER vent fan #4 air actuator cylinder body found wasted and air leaking.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Air actuator renewed, tested satisfactory","2020-01-02T23:59:35","","Completed","2020-01-02T23:59:35","No","No","No","Internal"]
[null,null,null,9871,null,"45_17/01/2020 1:36:26 PM","2020-01-16T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Hydraulic leak from the cylinder associated with engaging lever for STBD Windlass","Deck - Mooring Machinery","Mooring","Equipment Related,External Factors","9.2","Very High","","","Cylinder renewed. Leak rectified.","2020-01-20T23:59:35","","Completed","2020-01-17T23:59:35","No","No","No","Internal"]
[null,null,null,10536,null,"45_16/02/2020 8:36:22 PM","2020-01-30T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Lips of Natural Vent flaps rubber packing near China passage corroded.","Accommodation,Miscellaneous","General Appearance","Equipment Related,Human Error","11.1","High","","","De-rusted & painted","2020-04-29T23:59:35","","Completed","2020-04-27T23:59:35","No","No","No","Internal"]
[null,null,null,10537,null,"45_16/02/2020 8:30:34 PM","2020-01-30T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Cover of Dustbins in common spaces found broken.","Critical Equip.,Miscellaneous","General Appearance","Equipment Related,Human Error","6.2","High","","","NEW DUST BINS PUT IN USE","2020-04-29T23:59:35","SCAN200036","Completed","2020-06-17T23:59:35","No","No","No","Internal","WVessel will receive the RO on 6th June."]
[null,null,null,10540,null,"45_16/02/2020 12:05:10 PM","2020-02-01T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Ship Staff Insp.","16 K steam inlet valve bonnet found slightly  leaking (before auto dump valve)","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Steam isolated and valve bonnet gasket renewed.","2020-02-05T23:59:35","","Completed","2020-02-02T23:59:35","No","No","No","Internal"]
[null,null,null,10538,null,"45_16/02/2020 11:33:30 AM","2020-02-03T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Melted grease / Oil collected in the steering gear save all tray. Understand as per ship staff same is from the chain coupling. Grease to renew and confirm leakage.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Coupling grease renewed, no leakages observed.","2020-05-10T23:59:35","","Completed","2020-02-20T23:59:35","No","No","No","Internal"]
[null,null,null,10539,null,"45_16/02/2020 12:01:12 PM","2020-02-03T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ME sump condition to improve by better purification.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.7","Medium","","","LO Purifier tamperature maintained at 95°C, and optumum feed.ME sump oil condition improved.","2020-05-11T23:59:35","","Completed","2020-06-30T23:59:35","No","No","No","Internal"]
[null,null,null,10541,null,"45_16/02/2020 11:44:36 AM","2020-02-03T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Main air bottle, oil marks. Same was reported closed last time but still oil marks are clearly visible.","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Air bottles cleaned and painted","2020-02-21T23:59:35","","Completed","2020-02-12T23:59:35","No","No","No","Internal"]
[null,null,null,10542,null,"45_16/02/2020 11:55:35 AM","2020-02-03T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Water cooler outside ECR dripping continuously.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Water fountain tap repaired and fitted back. not dripping.","2020-03-10T23:59:35","","Completed","2020-02-13T23:59:35","No","No","No","Internal"]
[null,null,null,10543,null,"45_16/02/2020 11:39:37 AM","2020-02-03T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Steering gear door lock to renew.","E/R - Air Comp.,E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Lock removed, repaired and fitted back, working satisfactory","2020-03-10T23:59:35","","Completed","2020-02-13T23:59:35","No","No","No","Internal"]
[null,null,null,10553,null,"45_18/02/2020 5:02:00 PM","2020-02-03T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Both Lifeboat lowering motor and nearby area has rust patches","Deck - Machinery","General Appearance","External Factors","11.1","High","","","de rusted & painted.","2020-05-11T23:59:35","","Completed","2020-05-16T23:59:35","No","No","No","Internal"]
[null,null,null,10555,null,"45_18/02/2020 5:06:47 PM","2020-02-03T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Stbd windlass gear case oil is contaminated with water.","Deck - Mooring Machinery","Mooring","External Factors,Human Error","9.14","Medium","","","Oil Renewed","2020-02-26T23:59:35","","Completed","2020-02-26T23:59:35","No","No","No","Internal"]
[null,null,null,10556,null,"45_18/02/2020 4:57:44 PM","2020-02-03T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Aft mooring winches canvas cover is torn, same to be renewed.","Deck - Mooring Machinery","General Appearance","External Factors","11.1","High","","","Canvas cover renewed","2020-02-27T23:59:35","","Completed","2020-02-15T23:59:35","No","No","No","Internal"]
[null,null,null,10557,null,"45_18/02/2020 5:08:12 PM","2020-02-03T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Fore peak store light fitting top to clean","Deck - Machinery","General Appearance","External Factors,Human Error","11.1","High","","","Cleaned","2020-03-26T23:59:35","","Completed","2020-02-14T23:59:35","No","No","No","Internal"]
[null,null,null,10552,null,"45_18/02/2020 4:59:16 PM","2020-02-11T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Ship Staff Insp.","Emergency CO2 release box for emergency DG is in corroded condition.","Deck - Machinery","General Appearance","External Factors,Human Error","11.1","High","","","Added in Refman for DD Repairs","2020-05-11T23:59:35","","Completed","2020-03-01T23:59:35","No","No","No","Internal","Job to be completed, after joining of fitter."]
[null,null,null,10554,null,"45_18/02/2020 5:03:52 PM","2020-02-11T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Ship Staff Insp.","Foam monitor near isolation valve no 1 leaking from the flange.","Deck - Machinery","General Appearance","External Factors,Human Error","11.1","High","","","Rectified","2020-02-26T23:59:35","","Completed","2020-02-24T23:59:35","No","No","No","Internal"]
[null,null,null,10746,null,"45_03/03/2020 12:11:48 PM","2020-02-22T23:59:35","Defect","Ship Staff","Ship Staff Insp.","During saturday routine test found Port lifeboat was not starting on #2 battery.","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.27","Medium","","","Battery renewed with old good spare battery, working satisfactory. RO wiill be raised for new battery.","2020-02-23T23:59:35","","Completed","2020-02-22T23:59:35","No","No","No","Internal"]
[null,null,null,11339,null,"45_30/03/2020 3:34:52 PM","2020-03-10T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Manifold Drip Tray Grattings need to be Derusted & Fully Painted .","Deck - Pipe / Fittings","General Appearance","External Factors,Human Error","6.2","High","","","Both side manifold gratings derusting & painting completed.","2020-09-30T23:59:35","","Completed","2020-09-05T23:59:35","No","No","No","Internal","Job in progress. Target date revised accordingly."]
[null,null,null,11342,null,"45_30/03/2020 3:42:52 PM","2020-03-10T23:59:35","Observation","Ship Staff","Ship Staff Insp.","E/room Vents found rusted.","Deck - Pipe / Fittings","General Appearance","External Factors,Human Error","6.2","High","","","de-rusted & Painted.","2020-06-10T23:59:35","","Completed","2020-04-27T23:59:35","No","No","No","Internal"]
[null,null,null,11343,null,"45_30/03/2020 3:41:00 PM","2020-03-10T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Funnel Casing found Faded","Deck - Pipe / Fittings","General Appearance","External Factors,Human Error","6.2","High","","","Funnel painting carried out. ","2020-06-10T23:59:35","","Completed","2020-07-18T23:59:35","No","No","No","Internal","Job already completed. Update it."]
[null,null,null,10854,null,"45_20/03/2020 11:57:56 AM","2020-03-12T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Lagging of steam line of OWS is very poorly placed. To renew.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Knowledge Based","10.19","Very High","","","Renewed lagging of OWS heating lines","2020-04-20T23:59:35","","Completed","2020-03-20T23:59:35","No","No","No","Internal"]
[null,null,null,10855,null,"45_20/03/2020 12:12:40 PM","2020-03-12T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Drain box near stbd side of COPT plateform, to clean and paint.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Human Error,Knowledge Based","10.19","Very High","","","cleaned and painted","2020-03-30T23:59:35","","Completed","2020-03-19T23:59:35","No","No","No","Internal"]
[null,null,null,10856,null,"45_20/03/2020 12:21:46 PM","2020-03-12T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Condenser by pass valve to renew. To order new valve","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Valve received .To renew                                                .Old valve eased up . New valve kept as spare                              ","2020-08-31T23:59:35","SCAN 200083","Completed","2020-08-24T23:59:35","No","No","No","Internal","valve to renew at next opportunity. As it is  a black out job"]
[null,null,null,10857,null,"45_20/03/2020 12:25:38 PM","2020-03-12T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","FWG ejector pump's suction pipe flange is salt soaked. To renew gasket and cleaned.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related,Knowledge Based","10.29","Medium","","","Gasket renewed , no leaks ","2020-03-30T23:59:35","","Completed","2020-03-21T23:59:35","No","No","No","Internal"]
[null,null,null,10858,null,"45_20/03/2020 12:44:50 PM","2020-03-12T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","DG FO supply pump no 2 to overhaul, leaking from seal.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Pump  overhauled, mechanical seal and bearing renewed.No leaks","2020-04-05T23:59:35","","Completed","2020-04-06T23:59:35","No","No","No","Internal"]
[null,null,null,10859,null,"45_20/03/2020 4:00:44 PM","2020-03-12T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","On deck various chains are in rusted condition. To derust and paint.","Deck - Pipe / Fittings","General Appearance","External Factors","6.2","High","","","de rusted & painetd","2020-05-03T23:59:35","","Completed","2020-04-29T23:59:35","No","No","No","Internal"]
[null,null,null,10860,null,"45_20/03/2020 4:02:42 PM","2020-03-12T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Area below U-bolt to derust and paint in loaded passage.","Deck - Pipe / Fittings","General Appearance","External Factors,Human Error","6.2","High","","","to derust & paint","2021-03-15T23:59:35","","Completed","2021-03-14T23:59:35","No","No","No","Internal","Job is in progress, Target date revised."]
[null,null,null,10861,null,"45_20/03/2020 4:08:03 PM","2020-03-12T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Midship store natural vent cover to clean and paint.","Deck - Pipe / Fittings","General Appearance","External Factors,Human Error","6.2","High","","","Cleaned.","2020-03-26T23:59:35","","Completed","2020-03-23T23:59:35","No","No","No","Internal"]
[null,null,null,10862,null,"45_20/03/2020 4:09:34 PM","2020-03-12T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Steam line main valve for slop tank on deck to paint, as same is in rusty condition.","Deck - Pipe / Fittings","General Appearance","External Factors,Human Error","6.2","High","","","de rusted & painted","2020-05-04T23:59:35","","Completed","2020-03-12T23:59:35","No","No","No","Internal"]
[null,null,null,10863,null,"45_20/03/2020 12:36:09 PM","2020-03-12T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","MGPS anode is just lying on floor. Proper securing arrangement to make","Miscellaneous","Eng. / Strg. Comp.","Behaviour Based,Human Error","10.29","Medium","","","MGPS anode shifted and secured in designated stand.","2020-03-29T23:59:35","","Completed","2020-03-19T23:59:35","No","No","No","Internal"]
[null,null,null,10864,null,"45_20/03/2020 12:09:11 PM","2020-03-12T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Frosting noted i nmeat room fish room.Manual defrosting by hot water to be carried out twice a month.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related,Knowledge Based","10.29","Medium","","","Manual defrosting have been done and same will be followed twice a month.","2020-03-27T23:59:35","","Completed","2020-03-17T23:59:35","No","No","No","Internal"]
[null,null,null,10865,null,"45_20/03/2020 12:39:27 PM","2020-03-12T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","No.2 ME canshaft L.O booster pump suction pressure gauge to renew. Even with Main L.O pump stopped, it is showing pressure.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related,Human Error,Knowledge Based","10.29","Medium","","","Pressure gauge renewed.","2020-03-27T23:59:35","","Completed","2020-03-19T23:59:35","No","No","No","Internal"]
[null,null,null,10866,null,"45_20/03/2020 4:05:38 PM","2020-03-12T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Forward store hatch cover to paint.","Deck - Pipe / Fittings","General Appearance","External Factors,Human Error","6.2","High","","","Derusted, 3 coats primer applied & painted.","2020-03-29T23:59:35","","Completed","2020-03-20T23:59:35","No","No","No","Internal"]
[null,null,null,10867,null,"45_20/03/2020 4:13:10 PM","2020-03-12T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Meat room, Fish room, veg room to arrange in better manner.","Accommodation","General Appearance","External Factors","6.2","High","","","Vessel received provisions for 2 months & almost all racks are full. All empty cartons removed & arranged the racks as practicable as possible.","2020-04-18T23:59:35","","Completed","2020-03-20T23:59:35","No","No","No","Internal"]
[null,null,null,11572,null,"45_30/04/2020 6:50:00 AM","2020-03-30T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Platform holding bolts of cranes to be renewed","Deck - Machinery","Structural Condn. / WT integrity ","External Factors","11.6","Medium","","","Based on the condition of the removed bolts, it is not required to renew the bolts. (Mail rcvd from suptd. on 18 May 2020).","2020-06-30T23:59:35","","Completed","2020-05-18T23:59:35","No","No","No","Internal"]
[null,null,null,11348,null,"45_07/04/2020 8:35:20 PM","2020-04-03T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Aux. Boiler # 2 exhaust pipe expansion joint found with crack.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Expansion joint to be replaced. RO raised.               Refman job created","2020-09-30T23:59:35","SCAN 200094","Completed","2020-07-30T23:59:35","Yes","No","No","Internal","Job Assigned to DD"]
[null,null,null,13518,null,"45_16/08/2020 9:10:30 AM","2020-04-04T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","ME LO pump breaker no.2 found heated up and on inspection Y phase of breaker found black","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","On inspection it was found that cradle spring was loose and this caused into overheating of the cradle as well. Upon receiving new cradle along with MCCB same was replaced by isolating the bus tie breaker for GSP no.2","2020-08-14T23:59:35","","Completed","2020-08-06T23:59:35","No","No","No","Internal"]
[null,null,null,11574,null,"45_01/05/2020 8:23:50 AM","2020-04-05T23:59:35","Defect","Ship Staff","Ship Staff Insp.","LT cooler (100% ) sea water inlet pipe line leaking at bend due to  material wastage/hole","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","The pipeline bend at the sea water outlet of LT cooler renewed with pre fabricated bend recieved from shore.","2020-04-20T23:59:35","","Completed","2020-04-17T23:59:35","No","No","No","Internal"]
[null,null,null,11575,null,"45_01/05/2020 8:30:28 AM","2020-04-06T23:59:35","Defect","Ship Staff","Suptd. Insp.","Atm. condenser Sea water oulet pipe bend found leaking due to material wastage /hole","Deck - Pipe / Fittings","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Sea water oulet piupe bend renewed with prefabricated bend received from shore workshop","2020-04-30T23:59:35","","Completed","2020-04-17T23:59:35","No","No","No","Internal"]
[null,null,null,11349,null,"45_07/04/2020 12:46:20 PM","2020-04-06T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Foundation bolts of AFT ETA sheared off whilst testing. 2 bolts were drilled off & re instated with new ones","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","External Factors","","","","","All bolts renewed","2020-07-06T23:59:35","","Completed","2020-06-14T23:59:35","No","No","No","Internal"]
[null,null,null,11467,null,"45_17/04/2020 8:33:14 AM","2020-04-13T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Auxiliary  Boiler#2 atomizing steam valve found leaking","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Valve replaced with spare, no leaks.","2020-04-15T23:59:35","","Completed","2020-04-14T23:59:35","No","No","No","Internal"]
[null,null,null,11573,null,"45_01/05/2020 8:10:56 AM","2020-04-15T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Fressh water generator#1 jacket water inlet/outlet butterfly valves are stuck and not able to operate with handle.","E/R - Aux. Mach.,E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Renewed both jacket water  inlet& outlet valve of FWG#1. ","2020-06-30T23:59:35","","Completed","2020-06-22T23:59:35","No","No","No","Internal"]
[null,null,null,12022,null,"45_02/06/2020 8:32:49 AM","2020-05-01T23:59:35","Observation","Ship Staff","Ship Staff Insp.","W.O INCINERATOR FURNACE REFRACTORY FOUND DAMAGED AT SOME AREA.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","REFRACTORY REPAIRED.","2020-05-15T23:59:35","","Completed","2020-05-08T23:59:35","No","No","No","Internal"]
[null,null,null,12023,null,"45_02/06/2020 8:44:50 AM","2020-05-10T23:59:35","Observation","Ship Staff","Ship Staff Insp.","COPT L.O COOLER #2 AND #2  S.W PRESSURE GAUGE FOUND FAULTY","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","PRESSURE GAUGE RENEWED","2020-05-30T23:59:35","","Completed","2020-05-14T23:59:35","No","No","No","Internal"]
[null,null,null,11919,null,"45_19/05/2020 3:14:16 AM","2020-05-11T23:59:35","Defect","Ship Staff","Ship Staff Insp.","ME unit #6 crankcase door found leaking ","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Crankcase door gasket renewed.","2020-05-15T23:59:35","","Completed","2020-05-13T23:59:35","No","No","No","Internal"]
[null,null,null,12019,null,"45_02/06/2020 9:22:23 AM","2020-05-12T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Chief engineer's office ship viewer computer not working.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Trouble shooting has been carried out as per office instructions, still found not working. CPU to be renewed.","2020-09-30T23:59:35","","Completed","2020-10-24T23:59:35","No","No","No","Internal"]
[null,null,null,11918,null,"45_19/05/2020 2:55:13 AM","2020-05-20T23:59:35","Defect","Ship Staff","Ship Staff Insp.","AE flow meter not working ","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Flowmeter renewed, found working satisfactory","2020-08-30T23:59:35","SCAN200105","Completed","2020-07-15T23:59:35","No","No","No","Internal"]
[null,null,null,12024,null,"45_02/06/2020 8:38:37 AM","2020-05-24T23:59:35","Defect","Ship Staff","Ship Staff Insp.","VACUUME TOILET LINE FOUND CHOCKE MAKING VACUUME TOILET SYSTEM IN OPERATIONAL.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","PIPE SECTIONS REMOVED AND PIPE CLEARED AND FITTED BACK. SYSTEM WORKING NORMAL.","2020-05-25T23:59:35","","Completed","2020-05-24T23:59:35","No","No","No","Internal"]
[null,null,null,12020,null,"45_02/06/2020 9:33:08 AM","2020-05-28T23:59:35","Defect","Ship Staff","Ship Staff Insp.","VECS O2% INDICATION NOT SHOWING CORRECTLY AND NONFLOW ALARM NOT WORKING.","Inert Gas","Cargo / Ballast Systems","Equipment Related","8.17","Low","","","VECS conrol box including O2 sensor renewed. System functioning normally.","2020-09-30T23:59:35","SCAN200112","Completed","2020-10-08T23:59:35","No","No","No","Internal"]
[null,null,null,12021,null,"45_01/06/2020 11:43:52 PM","2020-05-28T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Pressure lines / Return lines of winches (W1, W2, W3, W5 & W8) have thinned down &  W3 return line having pin hole.","Deck - Mooring Machinery","Mooring","External Factors,Human Error","","","","","All thinned downed & temporary repaired lines renewd at Yiu Lian ship yard","2020-09-30T23:59:35","","Completed","2020-11-09T23:59:35","No","No","No","Internal"]
[null,null,null,12770,null,"45_18/06/2020 2:40:13 AM","2020-06-09T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Emergency switch board - bus tie breaker UVT controller defective","Elect. Mach. & Equip.","Emgcy. Systems","Equipment Related","10.37","Medium","","","UVT renewed","2020-09-30T23:59:35","","Completed","2020-07-08T23:59:35","No","No","No","Internal"]
[null,null,null,12997,null,"45_01/07/2020 9:36:22 AM","2020-06-23T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","CCTV to be installed at various places - CCR, ECR, Eng Room, Bridge facing deck area.","Miscellaneous","Communication","Equipment Related","","","","","Equipments recieved, intallation preparation work to be done by ship staff.Installation to be done by shore technician","2020-09-30T23:59:35","","Completed","2020-09-19T23:59:35","No","No","No","Internal"]
[null,null,null,12998,null,"45_01/07/2020 2:23:37 AM","2020-06-30T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Port Provision crane minor oil leakage  observed from luffing cylinder seal","Deck - Machinery","General Appearance","Equipment Related","8.76","Medium","","","Luffing cylinder seal to be renewed. Job included in REFMAN","2020-09-30T23:59:35","SCAN200115","Completed","2020-07-31T23:59:35","No","No","No","Internal"]
[null,null,null,13519,null,"45_16/08/2020 9:26:01 AM","2020-07-07T23:59:35","Defect","Ship Staff","Ship Staff Insp.","MOS panel on MSBD found not working","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","Upon inspection TFT of MOS panel found faulty. Same was replaced with spare MOS panel and setup/commisioning done according to procedure given in manual.","2020-08-14T23:59:35","","Completed","2020-08-12T23:59:35","No","No","No","Internal"]
[null,null,null,13199,null,"45_18/07/2020 4:59:51 AM","2020-07-15T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","#1 A/E Fuel oil booster pump, found vibrating and leaking from seal, On opening up, found oil in armature of the motor.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Replaced with spare new motor, and pump replaced with spare overhauled pump. Tried out found satisfactory","2020-07-16T23:59:35","","Completed","2020-07-15T23:59:35","No","No","No","Internal"]
[null,null,null,13520,null,"45_16/08/2020 9:20:37 AM","2020-07-15T23:59:35","Defect","Ship Staff","Ship Staff Insp.","ME Aux blower no.1 motor not getting started in Auto","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","On troubleshooting it was found on delay timer H3BAN was malfunctioning. Same was replaced during stoppage of ME and tried out.","2020-07-31T23:59:35","","Completed","2020-07-25T23:59:35","No","No","No","Internal"]
[null,null,null,13295,null,"45_31/07/2020 9:16:22 AM","2020-07-17T23:59:35","Defect,Observation","Ship Staff","Ship Staff Insp.","During previous  discharge,moderate Steam leakage from bonet gasket of steam dumping valve was noticed.","E/R - Pipes/ valves & fittings","Cargo / Ballast Systems","Equipment Related","10.32","Very High","","","1. Drains before valve found shut, same opened to drain condensate from lines, and practice maintained, to keep drain open at sea, to avoid, damage of gasket due to hammering.                2.System depressurised, and bonet gasket renewed","2020-07-18T23:59:35","","Completed","2020-07-18T23:59:35","No","No","No","Internal"]
[null,null,null,13299,null,"45_31/07/2020 9:53:58 AM","2020-07-17T23:59:35","Defect,Observation","Ship Staff","Ship Staff Insp.","Vacuum pump found cutting in 4 times in 1 minute.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Vacuum toilet eductor opened up for inspection,found one bolt on flap loose, hence flap not sitting in place, and therefore loss of vacuum, same rectified,cleaned, and fit back, now working satisfactory.","2020-07-25T23:59:35","","Completed","2020-07-23T23:59:35","No","No","No","Internal"]
[null,null,null,13300,null,"45_31/07/2020 9:33:49 AM","2020-07-19T23:59:35","Breakdown,Defect,Observation","Ship Staff","Ship Staff Insp.","1. M.D.O Starboard manifold valve found seized .                                                               2.Dresser coupling on M.D.O line bolts found excessivelly rusted.                                          3. M.D.O storage tank valve found hard.","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","Equipment Related","6.7","High","","","1. Gear box of valve opened up, found gear broked, renewed valve with new spare.                       2.Dresser coupling bolts, replaced with new bolts.   3.Gear case, of M.D.O storage tank valve opened up, and found excessive rust, same cleaned, filled with new grease,and new gasket, eased up.","2020-07-19T23:59:35","","Completed","2020-07-20T23:59:35","No","No","No","Internal"]
[null,null,null,13296,null,"45_31/07/2020 10:06:22 AM","2020-07-20T23:59:35","Breakdown,Defect","Ship Staff","Ship Staff Insp.","VRCS pump found not developing pressure, and hydraullic valves not operating from remote position","Cargo Mach.,Deck - Machinery,Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","10.32","Very High","","","1. Found relief valve in open condition,and short cycling of oil taking place, same overhaulled.         2. unloader solenoid, actuating the relief valve, found without  supply, on investigating, found pcb of unloader valve, burnt, same rectified by soldering.now working satisfactory ","2020-07-20T23:59:35","","Completed","2020-07-20T23:59:35","No","No","No","Internal"]
[null,null,null,13297,null,"45_31/07/2020 9:00:59 AM","2020-07-23T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","After discharging, vessel at low draught, deck Seal low flow alram sounded, followed by low level alarm.Deck seal Pump casings found excessively hot and developing low   pressure of 2.3 bar .Pumps changed over and found no improvement.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","1. Since the  fault being common,  pipe sections opened up and checked for blockages  but found clear.                                                                      2. Both Deck Seal pumps opened up for inspection, and clarances measured, found to be satisfactory. Vanes found blocked with shells, and dirt, same cleaned with chemical ,Both pumps tried out, found working satisfactory, Both pumps developing 4.5 bar pressure.      ","2020-07-24T23:59:35","","Completed","2020-07-24T23:59:35","No","No","No","Internal"]
[null,null,null,13298,null,"45_31/07/2020 8:31:19 AM","2020-07-28T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","1.Found fuel rack stuck and engine found excessively speeding                                                               2.L.o condition/colour in the sump found deteorated/discoloured.                             ","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.27","Medium","","","1.Fuel pump overhauled, ,found , control sleeve teeth broken, same turned 180 deg .                       2.Relay HB36D1 found in poor condition ( stop solenoid)  same renewed.                                       3 L.o in both lifeboat engines renewed","2020-07-28T23:59:35","","Completed","2020-07-28T23:59:35","No","No","No","Internal"]
[null,null,null,13294,null,"45_01/08/2020 8:22:17 AM","2020-07-31T23:59:35","Other","Ship Staff","Ship Staff Insp.","Sewage overbaoard  discharge rate chart for DHT Scandinavia  is not endorsed by class","E/R - Aux. Mach.","Eng. / Strg. Comp.","Industry Issue","10.32","Very High","","","Endorsed copy pasted on sewage holding tank","2020-08-31T23:59:35","","Completed","2020-08-07T23:59:35","No","No","No","Internal","Endorsed copy has already been sent  to vessel."]
[null,null,null,13521,null,"45_16/08/2020 9:38:27 AM","2020-08-03T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","AC motor no.2 found making abnormal sound and vibration","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","AC compressor no.2 was found in stand still condition from long time and on changing over,it was found running proper for a week but after that it was found that abnormal sound and vibration is coming from NDE of motor. So it was stopped and changed over to no.1. Upon inspection/opening it was found that brinelling was there on motor bearings as it was in standstill condition for long time with tension on driving belts. So motor was overahuled and AC compressor oil renwal and routines. Same was tried out and found running smooth. ","2020-08-14T23:59:35","","Completed","2020-08-10T23:59:35","No","No","No","Internal"]
[null,null,null,13522,null,"45_16/08/2020 2:26:28 AM","2020-08-04T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","Bilge pump tried out and found mechanical seal leaking excessively.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Pump opened up for inspection, and renewed line bearing and mechanical seal.","2020-08-06T23:59:35","","Completed","2020-08-04T23:59:35","No","No","No","Internal"]
[null,null,null,13523,null,"45_16/08/2020 2:36:52 AM","2020-08-05T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","a)1 pc pipe bender found defective.                            b)2 pcs vacuum bucket found disfuntioning","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","a)Teflon, seals and piston fabricated, now working satisfactory. Now being used to fabricate/bend pipes.                                                         b) O-ring /seals renewed, now working satisfactory,being used in e/r for maintainance purpose.","2020-08-05T23:59:35","","Completed","2020-08-05T23:59:35","No","No","No","Internal"]
[null,null,null,13532,null,"45_16/08/2020 3:01:36 AM","2020-08-06T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","a)vacuum tiolet found chocked by using face tissue paper.                                                            b)pipes internal diameter, found reduced due to excessive deposit in pipes.                                   c)loss of vacuum in the system","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related,External Factors,Human Error,Inappropriate Procedure","10.32","Very High","","","a) various sections in e/r opened up, cleared.          b) 4 sections cleared with high pressure gun, before being fit back.                                             c) vacuum leakage found in upper deck toilet, leakage rectified.","2020-08-06T23:59:35","","Completed","2020-08-06T23:59:35","No","No","No","Internal"]
[null,null,null,13524,null,"45_16/08/2020 4:35:35 AM","2020-08-07T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","Hydraulic leak on deck during sts operation from mooring winch return line.","Deck - Mooring Machinery,Deck - Pipe / Fittings","Eng. / Strg. Comp.","Equipment Related","","","","","leak temporarily arrested, sinse vessel in port.New pipe fabricated , and fitted back after completion of 1st loading.","2020-08-07T23:59:35","","Completed","2020-08-09T23:59:35","No","No","No","Internal"]
[null,null,null,13525,null,"45_16/08/2020 4:45:13 AM","2020-08-07T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","# 1 HFO purifeed pump leaking from  mechanical seal after a couple of days of running.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Seal renewed,and put into use, working satisfactory","2020-08-08T23:59:35","","Completed","2020-08-08T23:59:35","No","No","No","Internal"]
[null,null,null,13526,null,"45_16/08/2020 6:26:07 AM","2020-08-09T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","a)# 1 fwg , found not building up sufficient vacuuum.                                                                    b)Short cyling of fresh water, through high salinity solenoid valve when shut.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","a)#1 fwg  eductor opened up for inspection, found holed at throat, bronze putty applied.            b) additional ball cock fitted in line and kept shut.","2020-08-12T23:59:35","","Completed","2020-08-12T23:59:35","No","No","No","Internal"]
[null,null,null,13527,null,"45_16/08/2020 5:00:04 AM","2020-08-10T23:59:35","Defect,Observation","Ship Staff","Ship Staff Insp.","Boiler water circulating pump #2 outlet valve found leaking from bonet gasket.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Depressurised and drained entire line, gasket renewed for both pump  discharge valves.","2020-08-11T23:59:35","","Completed","2020-08-11T23:59:35","No","No","No","Internal"]
[null,null,null,13528,null,"45_16/08/2020 6:54:07 AM","2020-08-10T23:59:35","Breakdown,Defect","Ship Staff","Ship Staff Insp.","a)Found drop in pressure on Lp side of main air compressor # 2 .                                                   b)Lp side relief valve found lifting                              c) Lp liner found scratching marks, dents. Piston crown top found dented .                              d)  Crankase l.o discoloured","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Opened up compressor, found lp side suction valve plate broken,same renewed with new spare, and lapped delivery valve plate and fitted.     b)Relief valve on Lp side renewed with new spare.                                                                                c) Lp liner opened up, straches smoothed lightly, with rough stone. piston rings found intact.                      d)L.O renewed and sump cleaned,                ","2020-08-13T23:59:35","","Completed","2020-08-13T23:59:35","No","No","No","Internal"]
[null,null,null,13529,null,"45_16/08/2020 9:55:00 AM","2020-08-11T23:59:35","Breakdown,Defect","Ship Staff","Ship Staff Insp.","AE FO circulating motor no.1 found making abnormal sound and vibration ","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","On changing over to stand by motors it was found making abnormal sound and vibration. Upon dismantelling the motor NDE bearing casing of motor was found loose and bearing was damage. Same was repaired and motor was overhauled. Tried out after installation and was found running properly.","2020-08-20T23:59:35","","Completed","2020-08-11T23:59:35","No","No","No","Internal"]
[null,null,null,13530,null,"45_16/08/2020 7:33:38 AM","2020-08-12T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","During routine check/firing of incinerator, found primary burner not firing.","E/R - Aux. Mach.,Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","primary burnerattached  pump opened up for inspection found                                                                                 a) valve seized  same eased up                                             b)  Filter fully chocked, same cleaned.  Now working satisfactory                                                           ","2020-08-14T23:59:35","","Completed","2020-08-14T23:59:35","No","No","No","Internal"]
[null,null,null,13531,null,"45_16/08/2020 7:02:55 AM","2020-08-13T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","When trying to chemical clean main air coolers, found 90 % of nozzles blocked on both air coolers","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Both Air cooler pipes, on which nozzles are fitted, removed from air coolers, nozzles cleared, and put back, gaskets renewed","2020-08-15T23:59:35","","Completed","2020-08-15T23:59:35","No","No","No","Internal"]
[null,null,null,13533,null,"45_16/08/2020 7:22:29 AM","2020-08-13T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","During routine maintanance ,was unable to isolate the A/E Backwash filter, suspecting  a)backwashing drain valve not holding, and oil from the mixing column head continiously  flowing back to the filter.                               b)change over  block mechanism o-ring leaking","E/R - Pipes/ valves & fittings,Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","a) System drained, and new valve fitted.                          b)Change over block found seized and was unable to pull out, same jacked, o-ring renewed, and fitted back.","2020-08-13T23:59:35","","Completed","2020-08-13T23:59:35","No","No","No","Internal"]
[null,null,null,13914,null,"45_04/09/2020 6:39:26 AM","2020-08-21T23:59:35","Breakdown,Defect","Ship Staff","Ship Staff Insp.","2  Sections of the Winch hydraullic return line found leaking","Deck - Mooring Machinery,Deck - Pipe / Fittings","Mooring","Equipment Related","","","","","2 New hydraullic line sectiones fabricated in workshop and fitted on deck","2020-08-23T23:59:35","","Completed","2020-08-22T23:59:35","No","No","No","Internal"]
[null,null,null,13915,null,"45_04/09/2020 7:01:37 AM","2020-08-22T23:59:35","Breakdown,Defect","Ship Staff","Ship Staff Insp.","a).# 1 HFO purifier found Excessive vibration during discharging.                                                                 b).Bowl found overflowing.","E/R - Purifier","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Purifier opened up for inspection , found bowl nut  loose. Major overhaul carried out, bearings renewed , O-rings renewed , Clearances , height checked, Axial Vibration checked, found to be satisfactory. Purifier boxed back and tried out, found satisfactory","2020-08-27T23:59:35","","Completed","2020-08-25T23:59:35","No","No","No","Internal"]
[null,null,null,13916,null,"45_04/09/2020 7:07:16 AM","2020-08-23T23:59:35","Breakdown,Observation","Ship Staff","Ship Staff Insp.","UV sterilizer found not functioning, uv sterilizer filter found  dirty.                          Mineralizer dolomite filter dirty,                                 ","E/R - Aux. Engine,Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","UV sterilizer made operational. Dolomite granules cleaned, UV filter renewed. ","2020-08-23T23:59:35","","Completed","2020-08-23T23:59:35","No","No","No","Internal"]
[null,null,null,13917,null,"45_05/09/2020 9:24:30 AM","2020-08-25T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","#2 HFO purifier, found overflowing, and excessive vibration while discharging. Also found excessive vibration from motor non drive end bearing","E/R - Purifier","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","a)Purifier opened up, bowl cleaned, new o-ring and seal ring fitted.                                                                    b)Non drive end bearing casing found worn out,new bearings fitted with shim insert in non drive end.                                                                            .c) Friction pads renewed.                                               .Purifier boxed back and tried out, found working satisfactory.                                                              ","2020-08-27T23:59:35","","Completed","2020-08-27T23:59:35","No","No","No","Internal"]
[null,null,null,16130,null,"45_27/09/2020 11:11:02 AM","2020-09-07T23:59:35","Defect","Ship Staff","Ship Staff Insp.","No.1 boiler water level SIPART controller found malfunctioning and was not able to cope up with the water required by boiler.This resulted in alarm and tripping of boiler.","E/R - Boiler,Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","SIPART controller YWAY value, SCDUR value found was not proper, same was changed and initilisation of SIPART carried out and upperstream band as well as lower stream band adjusted before initialisation. After initialisation it was tried out and found working satisfactory.","2020-09-15T23:59:35","","Completed","2020-09-11T23:59:35","No","No","No","Internal"]
[null,null,null,16131,null,"45_03/10/2020 2:04:49 PM","2020-09-18T23:59:35","Defect,Observation","Ship Staff","Ship Staff Insp.","# 1 economiser feed pump found not coping up,when running at anchorage","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","# 1 economiser feed pump overhaulled, with new bearing, mouth ring, mechanical seals, sleeve, o-ring ,gaskets and put into use, now running satisfactory while running at anchorage.","2020-09-22T23:59:35","","Completed","2020-09-22T23:59:35","No","No","No","Internal"]
[null,null,null,16132,null,"45_03/10/2020 1:55:02 PM","2020-09-19T23:59:35","Defect","Ship Staff","Engineering Audit","#1 M/E fo circulating pump found leaking from mechanical seal/abnormal vibration sounded when started same.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","previously overhauled,M/E  f.o circulating pump which was kept ready to use state , put into use, and found out that overhaulled  pump also leaking from the seal, both pumps overhauled with new bearings and seals. one put into use, now running satisfactory","2020-09-19T23:59:35","","Completed","2020-09-19T23:59:35","No","No","No","Internal"]
[null,null,null,16133,null,"45_27/09/2020 10:58:56 AM","2020-09-20T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","NO.1 IG Blower Main breaker at 440V feeder panel of MSBD found malfunctioning due to failure of holding coil. ","Cargo Mach.,Elect. Mach. & Equip.","Cargo / Ballast Systems","Equipment Related","10.32","Very High","","","Old breaker HiBL 403 NE removed and new breaker UPB 400H installed having same capacity of 400Amps and and shunt trip coil of 220V.","2020-09-30T23:59:35","","Completed","2020-09-24T23:59:35","No","No","No","Internal"]
[null,null,null,16134,null,"45_03/10/2020 2:21:17 PM","2020-09-29T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","# 2 FWG ejector pump found leaking from the seal ","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","#2 fwg ejector pump, overhaulled  with new bearings,mechanical seals, mouth rings and casing ring, sleeve and o-rings ","2020-09-30T23:59:35","","Completed","2020-09-30T23:59:35","No","No","No","Internal"]
[null,null,null,16805,null,"45_05/01/2021 11:48:27 AM","2020-10-22T23:59:35","Defect,Observation","Ship Staff","Ship Staff Insp.","#3 A/E ,oil consumption too high, and external jacket  water leakage from #5  head ","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","#3 A/E , # 1 unit  piston opened up for inspection , found piston rings butt  clearances inline.renewed piston rings . and # 5 head leakage rectified by renewing o-rings","2020-12-31T23:59:35","","Completed","2020-12-23T23:59:35","No","No","No","Internal"]
[null,null,null,16135,null,"45_17/12/2020 7:23:59 PM","2020-10-30T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Portable Fire extinquisher, from steering flat removed from place during DD due to installation of EGCS effluent water outlet panel ","LSA / FFA","Eng. / Strg. Comp.","Equipment Related","5.33","High","","","Fire extinquisher fitted back with new modified bracket","2020-12-30T23:59:35","","Completed","2020-11-12T23:59:35","No","No","No","Internal"]
[null,null,null,16136,null,"45_16/12/2020 2:13:58 PM","2020-11-02T23:59:35","Observation","Ship Staff","Ship Staff Insp.","EEBD removed from location during DD due to installation of VFD pumps","LSA / FFA","Eng. / Strg. Comp.","Equipment Related","5.44","High","","","EEBD Kept back in place with new braket fitted","2020-11-15T23:59:35","","Completed","2020-11-13T23:59:35","No","No","No","Internal"]
[null,null,null,16124,null,"45_18/11/2020 11:18:52 PM","2020-11-04T23:59:35","Defect,Observation","Ship Staff","Ship Staff Insp.","SAAB tank RADAR gauging system - SCD touch function found defective","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.12","Medium","","","Service engineer attended the vessel on 4th feb 2021. Rectified the problem.","2021-02-19T23:59:35","","Completed","2021-02-04T23:59:35","No","No","No","Internal"]
[null,null,null,16137,null,"45_16/12/2020 1:45:12 PM","2020-11-05T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Portable foam extinquisher on boiler platform found lashed with rope, and locking pin bracket damaged","LSA / FFA","Eng. / Strg. Comp.","Equipment Related","5.33","High","","","Locking pin bracket repaired","2020-12-15T23:59:35","","Completed","2020-12-07T23:59:35","No","No","No","Internal"]
[null,null,null,16144,null,"45_18/11/2020 11:23:27 PM","2020-11-12T23:59:35","Observation","Ship Staff","Ship Staff Insp.","WBT gauging system - Levelmaster - H8 communication failure alarm triggers frequently","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.12","Medium","","","As per service technician report, H8 utility software will be required to identify defect.","2020-11-21T23:59:35","","Completed","2020-11-20T23:59:35","No","No","No","Internal"]
[null,null,null,16806,null,"45_05/01/2021 12:28:43 PM","2020-11-14T23:59:35","Observation","Ship Staff","Ship Staff Insp.","17 different types of stem , water, f.o leaks in engine room originated after DD and found few defective pressure gauges/thermometers","E/R - Aux. Engine,E/R - Aux. Mach.,E/R - Boiler,E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","All leaks nipped up, by isolating various systems.    various pressure gauges in engine replaced with new spare.","2020-12-31T23:59:35","","Completed","2020-12-28T23:59:35","No","No","No","Internal"]
[null,null,null,16145,null,"45_08/12/2020 5:04:09 PM","2020-11-18T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Fire hydrant next to 2C leaking","Critical Equip.","Safety / LSA / FFA","Equipment Related","","","","","Hydrant valve leak rectified.","2020-12-15T23:59:35","","Completed","2020-11-29T23:59:35","No","No","No","Internal"]
[null,null,null,16128,null,"45_14/12/2020 11:30:37 AM","2020-11-19T23:59:35","Defect,Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Gap between pipe and deck house bulkhead, same on M/E and D/G  exhaust pipe penetration from Engine casing","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","Staging  erected and job completed","2021-01-31T23:59:35","","Completed","2021-01-25T23:59:35","No","No","No","Internal","Job to be planned in ballast voyage. Target date revised. Presently vessel in discharge port."]
[null,null,null,16138,null,"45_16/12/2020 1:53:10 PM","2020-11-19T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Ship Staff Insp.","Reserve Fuel oil level in emergency generator tank found below minimum mark","Critical Equip.,LSA / FFA","Eng. / Strg. Comp.","Equipment Related","10.35","Very High","","","Reserve fuel tank topped up to minimum mark to run for 18 hrs on full load condition in accordance with solas","2020-12-20T23:59:35","","Completed","2020-11-22T23:59:35","No","No","No","Internal"]
[null,null,null,16139,null,"45_08/12/2020 1:36:22 PM","2020-11-19T23:59:35","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Accommodation panel to clean off hand stain.","Accommodation","General Appearance","Behaviour Based","11.1","High","","","All panels of accommodation cleaned with soap and water.","2020-11-21T23:59:35","","Completed","2020-11-20T23:59:35","No","No","No","Internal"]
[null,null,null,16140,null,"45_08/12/2020 1:42:03 PM","2020-11-19T23:59:35","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Suez canal crew room bed curtain hanging loose","Accommodation","General Appearance","Behaviour Based","11.1","High","","","suez canal crew room bed curtain fixed.","2020-11-21T23:59:35","","Completed","2020-11-21T23:59:35","No","No","No","Internal"]
[null,null,null,16141,null,"45_08/12/2020 1:59:35 PM","2020-11-19T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Suez canal cabin weather tight door packing channel to chip and paint.","Accommodation","General Appearance","Inappropriate Procedure","11.17","Low","","","Suez canal cabin weather tight door packing channel chipped and painted.","2020-11-25T23:59:35","","Completed","2020-11-24T23:59:35","No","No","No","Internal"]
[null,null,null,16142,null,"45_08/12/2020 2:14:56 PM","2020-11-19T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Slop tank (P) steam pipe deck penetration pieces to derust and paint. ","Deck - Pipe / Fittings","Cargo / Ballast Systems","External Factors","8.5","Very High","","","Slop tank (P) steam pipe deck penetration pieces derusted and painted. ","2020-11-23T23:59:35","","Completed","2020-11-22T23:59:35","No","No","No","Internal"]
[null,null,null,16143,null,"45_08/12/2020 4:12:05 PM","2020-11-19T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","COT 4P dry check port cap holding wire broken.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Human Error","8.12","Medium","","","COT 4P dry check port cap holding wire renwed.","2020-11-30T23:59:35","","Completed","2020-11-22T23:59:35","No","No","No","Internal"]
[null,null,null,16146,null,"45_08/12/2020 4:28:03 PM","2020-11-19T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Helicopter safety toolbox-suggested keep equipment list in the box for cross check .","Critical Equip.","Cargo / Ballast Systems","Human Error","2.3","High","","","Helicopter safety toolbox equipment list kept in the box .","2020-11-25T23:59:35","","Completed","2020-11-22T23:59:35","No","No","No","Internal"]
[null,null,null,16147,null,"45_08/12/2020 4:36:00 PM","2020-11-19T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Mid ship store (P) ventilation duck at FWD froze.","Hull & Tanks","Cargo / Ballast Systems","Human Error","11.6","Medium","","","FWD  ventilation duck of Mid ship store (P) freed , greased, descaled and painted.","2020-12-15T23:59:35","","Completed","2020-12-05T23:59:35","No","No","No","Internal"]
[null,null,null,16148,null,"45_08/12/2020 4:41:58 PM","2020-11-19T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","COT 3P COW line under side rust spots to derust and paint.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Human Error","11.5","Medium","","","COT 3P COW line under side rust spots derusted and painted","2020-12-15T23:59:35","","Completed","2020-12-07T23:59:35","No","No","No","Internal"]
[null,null,null,16149,null,"45_08/12/2020 4:46:36 PM","2020-11-19T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Hydraulic valve box no.2 cover holding wing nuts missing.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Human Error","11.5","Medium","","","Hydraulic valve box no.2 cover holding fitted with new wing nuts.","2020-12-14T23:59:35","","Completed","2020-12-03T23:59:35","No","No","No","Internal"]
[null,null,null,16150,null,"45_08/12/2020 4:52:18 PM","2020-11-19T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Hydraulic valve box no.2 hyd oil inlet valve hand wheel broken.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","11.5","Medium","","","Hydraulic valve box no.2 hyd oil inlet valve hand wheel fitted.","2020-12-12T23:59:35","","Completed","2020-12-02T23:59:35","No","No","No","Internal"]
[null,null,null,16151,null,"45_08/12/2020 4:58:10 PM","2020-11-19T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Main deck cable next to no.2 COT(C) manhole hanging loose-to secure with cable ties to secure with adequate cable tie.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Human Error","11.5","Medium","","","Main deck cable next to no.2 COT(C) manhole tied and securired with adequate cable tie.","2020-12-03T23:59:35","","Completed","2020-11-28T23:59:35","No","No","No","Internal"]
[null,null,null,16152,null,"45_08/12/2020 5:10:31 PM","2020-11-19T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","All mooring winche oil case cap frozen and oil glass opaque.","Deck - Mooring Machinery","Mooring","Equipment Related","9.14","Medium","","","All mooring winche oil case cap freed greased and oil sight glass cleaned.","2020-12-14T23:59:35","","Completed","2020-12-04T23:59:35","No","No","No","Internal"]
[null,null,null,16153,null,"45_08/12/2020 5:14:23 PM","2020-11-19T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Bosun store davit SWL to paint with contrast (black) colour.","Deck - Machinery","General Appearance","Human Error","8.63","High","","","Bosun store davit SWL to painted with contrast (black) colour.","2020-12-16T23:59:35","","Completed","2020-12-03T23:59:35","No","No","No","Internal"]
[null,null,null,16154,null,"45_08/12/2020 5:20:04 PM","2020-11-19T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","F'cle deck dead man roller to SWL to paint with contrast colour(White).","Deck - Mooring Machinery","Mooring","Human Error","9.19","Low","","","F'cle deck dead man roller to SWL painted with contrast colour(White).","2020-12-15T23:59:35","","Completed","2020-12-05T23:59:35","No","No","No","Internal"]
[null,null,null,16155,null,"45_08/12/2020 4:19:22 PM","2020-11-19T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","FO bunker manifold (P) FWD pressure guage showing 3.5 bars although bunker recived from STBD side. Pls check whether valve is leaking or pressure guage is defective and take necessary action.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Human Error","6.7","High","","","The pipe fitted to the pressure guage found choked same cleaned and fitted back.","2020-11-25T23:59:35","","Completed","2020-11-21T23:59:35","No","No","No","Internal"]
[null,null,null,16156,null,"45_08/12/2020 5:26:51 PM","2020-11-19T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Bosun store local fire-fighting system start panel blocked.","Critical Equip.","Safety / LSA / FFA","Human Error","5.4","High","","","Bosun store local fire-fighting system start panel block cleared.","2020-11-26T23:59:35","","Completed","2020-11-21T23:59:35","No","No","No","Internal"]
[null,null,null,16157,null,"45_08/12/2020 6:02:34 PM","2020-11-19T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Life buoys kept in bosun stores.","LSA / FFA","Safety / LSA / FFA","Human Error","5.31","High","","","Life buoys kept in their respective places.","2020-11-21T23:59:35","","Completed","2020-11-20T23:59:35","No","No","No","Internal"]
[null,null,null,16158,null,"45_08/12/2020 6:06:43 PM","2020-11-19T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","One spare valve lying near mast riser -to shift to mid ship store.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Human Error","5.11","Low","","","One spare valve lying near mast riser shifted to mid ship store.","2020-12-01T23:59:35","","Completed","2020-11-26T23:59:35","No","No","No","Internal"]
[null,null,null,16159,null,"45_08/12/2020 6:13:09 PM","2020-11-19T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Pump room housekeeping to improve.Metal scraps, chain etc lying on tank top.","Cargo Mach.","Cargo / Ballast Systems","Human Error","8.51","Low","","","Pump room cleaned and removed Metal scraps, chain etc lying on tank top .","2020-12-10T23:59:35","","Completed","2020-12-08T23:59:35","No","No","No","Internal"]
[null,null,null,16160,null,"45_08/12/2020 6:20:10 PM","2020-11-19T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Mooring winch M12 platform lip wasted.","Deck - Mooring Machinery","Mooring","External Factors","9.14","Medium","","","Mooring winch M12 platform lip damage cleared.","2020-12-15T23:59:35","","Completed","2020-12-07T23:59:35","No","No","No","Internal"]
[null,null,null,16161,null,"45_08/12/2020 6:23:49 PM","2020-11-19T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Gymnasium untidy","Accommodation","General Appearance","Human Error","11.1","High","","","Gymnasium cleaned and arranged.","2020-12-13T23:59:35","","Completed","2020-12-03T23:59:35","No","No","No","Internal"]
[null,null,null,16162,null,"45_08/12/2020 6:29:28 PM","2020-11-19T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Pump room EEBD box cover brocken.","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.27","Medium","","","Pump room EEBD box cover fixed.","2020-12-13T23:59:35","","Completed","2020-12-04T23:59:35","No","No","No","Internal"]
[null,null,null,16163,null,"45_09-Dec-20 1:45:08 AM","2020-11-19T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Notice board pen holder filled with trash.","Accommodation","General Appearance","Behaviour Based","11.1","High","","","Removed trash from notice board pen holder. ","2020-11-22T23:59:35","","Completed","2020-11-20T23:59:35","No","No","No","Internal"]
[null,null,null,16164,null,"45_09-Dec-20 1:48:19 AM","2020-11-19T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Deck above paint lock to derust and paint.","Accommodation","General Appearance","External Factors","11.1","High","","","Derusted and painted on deck above paint locker. ","2020-12-15T23:59:35","","Completed","2020-12-08T23:59:35","No","No","No","Internal"]
[null,null,null,16165,null,"45_09-Dec-20 1:56:33 AM","2020-11-19T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","EGCS deck house fire extinguishers to be included in firefighting equipment booklet and also tag for monthly condition check to attach.","LSA / FFA","Safety / LSA / FFA","Human Error","5.27","Medium","","","EGCS deck house fire extinguishers included in firefighting equipment booklet and also taged for monthly condition and attached.","2020-11-26T23:59:35","","Completed","2020-11-22T23:59:35","No","No","No","Internal"]
[null,null,null,16166,null,"45_09-Dec-20 2:00:12 AM","2020-11-19T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Engine casing at aft stained - to clean and paint.","Accommodation","General Appearance","External Factors","11.1","High","","","Engine casing at aft cleaned and painted.","2020-12-15T23:59:35","","Completed","2020-12-07T23:59:35","No","No","No","Internal"]
[null,null,null,16167,null,"45_09-Dec-20 2:05:31 AM","2020-11-19T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Cable tray joining bracket missing at few laocations.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Human Error","11.5","Medium","","","Cable tray joining bracket fixed back.","2020-12-07T23:59:35","","Completed","2020-11-27T23:59:35","No","No","No","Internal"]
[null,null,null,16168,null,"45_09-Dec-20 1:51:42 AM","2020-11-19T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","FO tank save all tray (next to pump room entrance P) plug missing.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Human Error","8.12","Medium","","","FO tank save all tray (next to pump room entrance P) pluged.","2020-11-23T23:59:35","","Completed","2020-11-21T23:59:35","No","No","No","Internal"]
[null,null,null,16169,null,"45_12/12/2020 1:10:09 PM","2020-11-19T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Loose slings on top of BWTS filters in pump room to secure.","Cargo Mach.","Cargo / Ballast Systems","Human Error","5.11","Low","","","Loose slings on top of BWTS filters in pump room secured","2020-11-22T23:59:35","","Completed","2020-11-21T23:59:35","No","No","No","Internal"]
[null,null,null,16170,null,"45_20/12/2020 10:22:21 AM","2020-11-19T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","LT cooler gaskets stowed in box . Its likelythat gaskets will be permanently deformed at the bend and crack.","E/R - Pipes/ valves & fittings,Miscellaneous","Eng. / Strg. Comp.","Equipment Related,Inappropriate Procedure","10.32","Very High","","","New stand fabricated for stowing gaskets , to prevent from twisting of gaskets","2020-11-30T23:59:35","SCAN200112","Completed","2020-11-25T23:59:35","No","No","No","Internal"]
[null,null,null,16171,null,"45_20/12/2020 10:44:48 AM","2020-11-19T23:59:35","Defect,Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Bulkhead insulation covering aft of  D/G#2 exhaust uptake to repair","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Human Error","10.32","Very High","","","New insulation fitted at aft portion of D/G # 2 uxhaust uptake","2020-12-30T23:59:35","","Completed","2020-11-26T23:59:35","No","No","No","Internal"]
[null,null,null,16172,null,"45_20/12/2020 10:52:39 AM","2020-11-19T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Boiler water circulating pump pressure gauges hanging loose","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Boiler water circulating pump and other pumps pressure gauges  secured","2020-11-30T23:59:35","","Completed","2020-11-21T23:59:35","No","No","No","Internal"]
[null,null,null,16173,null,"45_20/12/2020 11:11:28 AM","2020-11-19T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Ship Staff Insp.","#5 Aft fuel injector return line pipe slight leakage from union","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.19","Very High","","","Union tightened and leak rectified","2020-11-21T23:59:35","","Completed","2020-11-20T23:59:35","No","No","No","Internal"]
[null,null,null,16174,null,"45_11/12/2020 10:22:38 PM","2020-11-19T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Main deck cable tray support bracket rusted ,to derust and paint.","Deck - Pipe / Fittings","Cargo / Ballast Systems","External Factors","11.5","Medium","","","Main deck cable tray support bracket derusted and painted.","2020-12-12T23:59:35","","Completed","2020-11-28T23:59:35","No","No","No","Internal"]
[null,null,null,16175,null,"45_20/12/2020 1:06:51 PM","2020-11-19T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Scavenge air cooler (aft) cooling water outlet valve handle missing","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","New handle fitted","2020-12-19T23:59:35","","Completed","2020-11-22T23:59:35","No","No","No","Internal"]
[null,null,null,16176,null,"45_20/12/2020 1:17:30 PM","2020-11-19T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Sewage plant tray to derust & paint","Miscellaneous","General Appearance","External Factors","10.32","Very High","","","Sewage plant tray painting carried out.","2020-12-19T23:59:35","","Completed","2020-11-22T23:59:35","No","No","No","Internal"]
[null,null,null,16177,null,"45_20/12/2020 1:22:04 PM","2020-11-19T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ODME Oil content meter air leakage","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","6.13","Low","","","Pipe fittings renewed","2020-12-20T23:59:35","","Completed","2020-11-22T23:59:35","No","No","No","Internal"]
[null,null,null,16178,null,"45_20/12/2020 1:02:15 PM","2020-11-19T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","M/E T/C (aft) manometer water level not visible","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Manometer filled with water.","2020-12-15T23:59:35","","Completed","2020-11-22T23:59:35","No","No","No","Internal"]
[null,null,null,16179,null,"45_20/12/2020 1:29:39 PM","2020-11-19T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","LO drain filter vent valve hand wheel missing","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","New handwheel fitted","2020-11-28T23:59:35","","Completed","2020-11-22T23:59:35","No","No","No","Internal"]
[null,null,null,16180,null,"45_20/12/2020 1:36:36 PM","2020-11-19T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Stern tube oil tank level less then normal mark","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Oil topped up.","2020-11-30T23:59:35","","Completed","2020-11-22T23:59:35","No","No","No","Internal"]
[null,null,null,16181,null,"45_20/12/2020 1:32:57 PM","2020-11-19T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Scavenge air cooler drain pipe sight glass dirty.","E/R - Main Engine","General Appearance","Equipment Related","10.32","Very High","","","Sight glass cleaned.","2020-11-30T23:59:35","","Completed","2020-11-22T23:59:35","No","No","No","Internal"]
[null,null,null,16182,null,"45_20/12/2020 1:39:06 PM","2020-11-19T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Engine room tank top aft of flywheel area to clean","Miscellaneous","General Appearance","External Factors","10.29","Medium","","","Area cleaned of oil and water","2020-11-30T23:59:35","","Completed","2020-11-22T23:59:35","No","No","No","Internal"]
[null,null,null,16183,null,"45_20/12/2020 1:41:40 PM","2020-11-19T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ME unit 3 cam space covered with oil","E/R - Main Engine","General Appearance","Equipment Related","10.19","Very High","","","Camspace space cleaned and source of leak rectified.","2020-11-22T23:59:35","","Completed","2020-11-22T23:59:35","No","No","No","Internal"]
[null,null,null,16190,null,"45_20/12/2020 1:45:26 PM","2020-11-19T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Metal scraps lying in the funnel space.","Miscellaneous","General Appearance","Human Error","10.29","Medium","","","Metal scrap removed and area cleaned","2020-11-30T23:59:35","","Completed","2020-11-22T23:59:35","No","No","No","Internal"]
[null,null,null,16125,null,"45_11/12/2020 10:17:21 PM","2020-11-19T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Various Pipes on main deck have rust spots.pipe to derust to chip.","Deck - Pipe / Fittings","Cargo / Ballast Systems","External Factors","8.3","Very High","","","To derust and paint","2021-03-16T23:59:35","","Completed","2021-03-13T23:59:35","No","No","No","Internal","Job in progress. Target date revised."]
[null,null,null,16126,null,"45_11/12/2020 10:25:44 PM","2020-11-19T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Few deck pipe U clamp rusted , to renew.","Deck - Pipe / Fittings","Cargo / Ballast Systems","External Factors","8.3","Very High","","","Renew rusted U clamps.","2021-02-16T23:59:35","","Completed","2021-01-12T23:59:35","No","No","No","Internal","Job in progress. Target date revised."]
[null,null,null,16127,null,"45_11/12/2020 10:30:11 PM","2020-11-19T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Main deck spot rusts to derust and paint.","Hull & Tanks","Cargo / Ballast Systems","External Factors","11.1","High","","","Spot derusting & painting of main deck area completed.","2021-04-30T23:59:35","","Completed","2021-04-08T23:59:35","No","No","No","Internal","Job is progress. Target date revised."]
[null,null,null,16184,null,"45_17/12/2020 7:44:18 PM","2020-11-28T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Main engine # 6 cylinder lubricator found scoring marks on plungers when previously opend up in DD by servive engineer.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Same renewed with new spare received and lubrication checked, found to be satisfactory","2020-12-08T23:59:35","","Completed","2020-11-29T23:59:35","No","No","No","Internal"]
[null,null,null,16185,null,"45_16/12/2020 2:20:44 PM","2020-12-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Both main air compressors 1 and 2, stud found broken on LP and HP side respectively","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Both compressor, cylinder heads removed. broken studs, drilled and removed using stud extractor.","2020-12-03T23:59:35","","Completed","2020-12-02T23:59:35","No","No","No","Internal"]
[null,null,null,16186,null,"45_17/12/2020 7:35:53 PM","2020-12-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Oil leaking from seal of turning gear","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Gear wheel removed from place and new oil seal renewed.","2020-12-03T23:59:35","","Completed","2020-12-02T23:59:35","No","No","No","Internal"]
[null,null,null,16189,null,"45_16/12/2020 2:27:42 PM","2020-12-02T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","#2 Hfo Purifier found slightly vibrating","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","#2 Hfo purifier opened up for inspection, bowl cleaned, found, bown nut loose, same cleaned and bowl nut tightened @ 100 n-m ","2020-12-05T23:59:35","","Completed","2020-12-04T23:59:35","No","No","No","Internal"]
[null,null,null,16187,null,"45_17/12/2020 7:14:31 PM","2020-12-05T23:59:35","Defect,Observation","Ship Staff","Ship Staff Insp.","Galley overboard pipe section before overboardvalve found holed, and water leaking into engine room","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","New pipe fabricated and fitted back","2020-12-07T23:59:35","","Completed","2020-12-07T23:59:35","No","No","No","Internal"]
[null,null,null,16188,null,"45_07/12/2020 7:37:20 PM","2020-12-06T23:59:35","Breakdown,Observation","Ship Staff","Ship Staff Insp.","Upper deck common toilet flush non functional.Toilet kept untidy .","Accommodation","MLC Related","Equipment Related","11.13","Low","","","On troubleshooting found that control valve and water valve malfunctioning. Same repaired and fitted back. Working satisfactorily.Toilet cleaned ","2020-12-25T23:59:35","","Completed","2020-12-07T23:59:35","No","No","No","Internal"]
[null,null,null,11340,null,"45_30/03/2020 3:38:19 PM","2020-12-10T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Gangways Operating area need to be Guarded.","Deck - Pipe / Fittings","General Appearance","External Factors,Human Error","6.2","High","","","Need to get Guard fabricated onboard ship's workshop.","2021-01-30T23:59:35","","Completed","2021-01-14T23:59:35","Yes","No","No","Internal"]
[null,null,null,16807,null,"45_05/01/2021 1:06:03 PM","2020-12-15T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Ingress of condensate water found in Engine room service air line.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Aux boiler no.2 atomising air valve found leaking,non return check valve spring found damaged,same replaced with sapre.Ball valve seal and packing replaced with new spare","2020-12-31T23:59:35","","Completed","2020-12-30T23:59:35","No","No","No","Internal"]
[null,null,null,11347,null,"45_07/04/2020 8:29:13 PM","2020-12-19T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Inventory management: All spare parts to be checked, varified and update in PAL with correct storing location.","Documentation","ISM Related","Equipment Related","10.12","Very High","","","All spare parts to be checked, varified and update in PAL with correct storing location.Job in progress","2021-03-25T23:59:35","","Completed","2021-03-25T23:59:35","No","No","No","Internal"]
[null,null,null,16808,null,"45_05/01/2021 2:36:06 PM","2020-12-23T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","UV Sterilizer giving abnormal alarm","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","On inspection it was found ballast was burnt and not working and UV light glass found broken. Same was renewed and new ballast installed from pump room light. Since these are not being used as we have converted it into LEDs","2021-01-31T23:59:35","","Completed","2020-12-24T23:59:35","No","No","No","Internal"]
[null,null,null,16809,null,"45_03/01/2021 11:34:43 AM","2020-12-27T23:59:35","Defect","Ship Staff","Ship Staff Insp.","#1 fwg ejector pump found leaking from the seal","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","# 1 FWG Pump opened up for inspection and seal renewed.anodes found completly wasted and pump casing corroded,same rectified by cold repair.Pump motor overhauled both ends bearings replaced with new spare.","2020-12-31T23:59:35","","Completed","2020-12-30T23:59:35","No","No","No","Internal"]
[null,null,null,17713,null,"45_25/01/2021 9:43:06 AM","2021-01-04T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","#1 Main air compressor, coupling found broken ","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Motor removed from place, renewed new gear and coupling. Tried out, now running satisfactory.","2021-01-05T23:59:35","","Completed","2021-01-04T23:59:35","No","No","No","Internal"]
[null,null,null,17714,null,"45_25/01/2021 11:25:48 AM","2021-01-05T23:59:35","Observation","Ship Staff","Ship Staff Insp.","#1 Refregeration compressor overhauling record not found. Mechanical seal found leaking","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Refregeration compressor overhauled with new spares, piston , con rod and mechanical seal renewed. tried out found satisfactory","2021-01-16T23:59:35","","Completed","2021-01-15T23:59:35","No","No","No","Internal"]
[null,null,null,16804,null,"45_05/01/2021 2:25:19 PM","2021-01-14T23:59:35","Breakdown,Critical Equipment","Ship Staff","Ship Staff Insp.","OWS found not starting.On inspection it was found PLC is showing error 6401.It means it is having sum check error.","Critical Equip.","MARPOL Related","Equipment Related","","","",""," RO 215009 raised for service attendance. Technician attended the vessel on 4 FEB 21, renewed the PLC with new spare, set the timer values. Found the system working satisfactory.","2021-01-31T23:59:35","","Completed","2021-02-04T23:59:35","No","No","No","Internal"]
[null,null,null,17712,null,"45_25/01/2021 8:47:21 PM","2021-01-15T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Salinometer found malfunctioning at cascade tank","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","salinometer changed with new spare.","2021-05-15T23:59:35","","Completed","2021-04-11T23:59:35","No","No","No","Internal"]
[null,null,null,17715,null,"45_25/01/2021 11:32:22 AM","2021-01-15T23:59:35","Breakdown,Defect","Ship Staff","Ship Staff Insp."," Inert gas  high temperature  sensor  found corroded, leading to tripping of IG plant","Inert Gas","Eng. / Strg. Comp.","Equipment Related","8.3","Very High","","","Spare IG sensor fitted, now working satisfactory","2021-02-15T23:59:35","","Completed","2021-01-25T23:59:35","No","No","No","Internal"]
[null,null,null,17716,null,"45_25/01/2021 7:49:30 PM","2021-01-22T23:59:35","Breakdown,Defect","Ship Staff","Ship Staff Insp.","#1 main air compressor, 2 LP side studs found broken","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","All four studs on LP Side renewed with new studs","2021-01-23T23:59:35","","Completed","2021-01-22T23:59:35","No","No","No","Internal"]
[null,null,null,18205,null,"45_03/03/2021 3:43:54 PM","2021-02-04T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Paint peel of @ several places on main deck","Hull & Tanks","General Appearance","External Factors","11.1","High","","","All loose paint removed on main deck from Midship to Accomodation block & Re-painted with 2 coats of primer followed by top coat.","2021-05-03T23:59:35","","Completed","2021-05-02T23:59:35","No","No","No","Internal"]
[null,null,null,18206,null,"45_09/03/2021 11:52:56 PM","2021-02-04T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Aft FWG evaporator plates leaking.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Evaporatot side gaskets renewed with sapre new gasket and leakage rectified.","2021-04-30T23:59:35","SCAN210044","Completed","2021-04-10T23:59:35","No","No","No","Internal"]
[null,null,null,18207,null,"45_13/03/2021 5:06:07 PM","2021-02-04T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","EGCS RECORD BOOK NOT MAINTAINED","Documentation","MARPOL Related","Equipment Related","10.11","Medium","","","EGCS PARAMETES READINGS ARE RECORDED IN ENGINE ROOM LOG BOOK AND FULL PARAMETER READINGS ARE DOWLOADED  FROM EGCS PANEL AND RECORDED SEPARATELY IN COMPUTER. AWATING FOR EGCS RECORD BOOK. ","2021-04-30T23:59:35","","Completed","2021-03-24T23:59:35","No","No","No","Internal"]
[null,null,null,18208,null,"45_03/03/2021 3:54:03 PM","2021-02-04T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Windlass brake adjustment – match marking not there.","Deck - Mooring Machinery","Mooring","Equipment Related","9.14","Medium","","","Windlass brake adjustment – match marking.","2021-03-07T23:59:35","","Completed","2021-03-06T23:59:35","No","No","No","Internal"]
[null,null,null,18209,null,"45_09/03/2021 11:43:13 PM","2021-02-04T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ME lube oil purifier operated at 71 degree celsius inlet temperature","E/R - Purifier","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","ME lube oil purifier operating temperature adjusted to 92 degree celsius.","2021-02-14T23:59:35","","Completed","2021-02-05T23:59:35","No","No","No","Internal"]
[null,null,null,18210,null,"45_09/03/2021 11:45:39 PM","2021-02-04T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","All cargo pumps bulkhead seal grease level low.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.45","High","","","All cargo pumps bulkhead seal grease topped up full.","2021-02-14T23:59:35","","Completed","2021-02-10T23:59:35","No","No","No","Internal"]
[null,null,null,18211,null,"45_09/03/2021 11:48:21 PM","2021-02-04T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Steam leak from no:-1 HFO purifier temp control valve.","E/R - Purifier","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Temp control valve spindle bush tightened and steam leakage rectified.","2021-03-04T23:59:35","","Completed","2021-02-08T23:59:35","No","No","No","Internal"]
[null,null,null,18212,null,"45_10/03/2021 12:01:11 AM","2021-02-04T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ME LO auto back wash filter aft chamber rotation is slow","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","ME LO auto back wash filter driving hydraulic motor overhauled, found wear and tear in driving slots, defective spare changed and tried out, found in good order.","2021-04-04T23:59:35","","Completed","2021-03-05T23:59:35","No","No","No","Internal"]
[null,null,null,18213,null,"45_10/03/2021 12:10:19 AM","2021-02-04T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","EGCS room need cleaning","Miscellaneous","General Appearance","Equipment Related","10.29","Medium","","","EGCS room cleaning completed.","2021-03-04T23:59:35","","Completed","2021-02-24T23:59:35","No","No","No","Internal"]
[null,null,null,18214,null,"45_10/03/2021 12:18:38 AM","2021-02-04T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Lamp fused in emergency escape","Elect. Mach. & Equip.","Safety / LSA / FFA","Equipment Related","10.15","Low","","","Lamp changed with spare lamp.","2021-02-09T23:59:35","","Completed","2021-02-04T23:59:35","No","No","No","Internal"]
[null,null,null,18215,null,"45_03/03/2021 3:36:44 PM","2021-02-04T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","IG pipe section near deck seal vent has signs of leakage.","Deck - Pipe / Fittings","General Appearance","External Factors","8.23","Medium","","","No leaks found.","2021-03-20T23:59:35","","Completed","2021-03-13T23:59:35","No","No","No","Internal"]
[null,null,null,18216,null,"45_10/03/2021 12:05:45 AM","2021-02-04T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Oil sheen in aft bilge well","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Aft bilge well cleaning to be carriedout.","2021-04-04T23:59:35","","Completed","2021-03-04T23:59:35","No","No","No","Internal"]
[null,null,null,18087,null,"45_01/03/2021 7:27:45 PM","2021-02-28T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Required new plate gaskets for no.1 fresh water generator.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Defective gaskets renewed with new gasket.","2021-04-01T23:59:35","SCAN210044","Completed","2021-04-10T23:59:35","No","No","No","Internal"]
[null,null,null,18460,null,"45_31/03/2021 9:35:31 PM","2021-03-25T23:59:35","Defect","Ship Staff","Ship Staff Insp.","starboard grey water line in engine room bottom platform found leaking from seam.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","permanent repair carried out by renewing the pipe.","2021-04-30T23:59:35","","Completed","2021-04-06T23:59:35","No","No","No","Internal"]
[null,null,null,18459,null,"45_31/03/2021 9:23:39 PM","2021-03-31T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","Fwd piston horn found not  working, same opened for inspection, piston and connecting rod broken in to small peices and liner got damaged due to broken connecting rod and piston","Navigation - Others","Communication","Equipment Related","12.12","High","","","All damaged parts renewed and tried out.","2021-05-31T23:59:35","","Completed","2021-04-01T23:59:35","No","No","No","Internal"]
[null,null,null,9594,null,"45_12/01/2020 9:55:38 AM","2021-04-03T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Aux boiler no:-2 aux feed water line auto control valve gland seal is leaking.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Auto control valve gland seal renew with new gland seal kit and leakage rectified.","2021-04-25T23:59:35","","Completed","2021-04-14T23:59:35","No","No","No","Internal","Job in progress, Target date revised accordingly."]
[null,null,null,18979,null,"45_30/04/2021 2:38:01 PM","2021-04-09T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","M14 mooring winch, operating control unit hydralic pipe line uniion connection found leaking.","Deck - Pipe / Fittings","Mooring","Equipment Related","9.14","Medium","","","Defective union connections renewed and leakage rectified.","2021-05-30T23:59:35","","Completed","2021-05-01T23:59:35","No","No","No","Internal"]
[null,null,null,18980,null,"45_30/04/2021 2:43:39 PM","2021-04-09T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Windlass stbd hydraulic block pipe connection leaking.","Deck - Machinery","Mooring","Equipment Related","9.14","Medium","","","O-ring renewed for the flange connections and leakage rectified.","2021-05-30T23:59:35","","Completed","2021-05-03T23:59:35","No","No","No","Internal"]
[null,null,null,19500,null,"45_03/05/2021 20:00:30","2021-04-09T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Insulation matt in front of electrical panels in bosun store missing","Miscellaneous","General Appearance","Behaviour Based","10.24","Low","","","Insulation matt placed in front of electrical panel in bosun store.","2021-04-24T23:59:35","","Completed","2021-04-15T23:59:35","No","No","No","Internal"]
[null,null,null,19501,null,"45_03/05/2021 20:19:29","2021-04-09T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Air Con compressor no. 2 suction & discharge pressure gauge defective","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","External Factors","10.32","Very High","","","Defective gauge replaced with new spare.","2021-05-08T23:59:35","","Completed","2021-04-18T23:59:35","No","No","No","Internal"]
[null,null,null,19502,null,"45_03/05/2021 20:21:31","2021-04-09T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","LT cooler no 1 & 2 SW inlet flange slight leakage / covered with salt\n\n","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","External Factors","10.31","Very High","","","Flange disconnected, gasket renewed and leakage rectified..","2021-06-08T23:59:35","","Completed","2021-04-30T23:59:35","No","No","No","Internal"]
[null,null,null,19503,null,"45_03/05/2021 20:24:16","2021-04-09T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Rubber matt in front of EGCS remote I/O cabinet missing","E/R - Pumps","General Appearance","Behaviour Based,Human Error","10.24","Low","","","Rubber mat placed in front of EGCS remote cabinet.","2021-05-23T23:59:35","","Completed","2021-04-19T23:59:35","No","No","No","Internal"]
[null,null,null,19504,null,"45_03/05/2021 20:26:16","2021-04-09T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","440V feeder circuit resistance less than infinity","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Behaviour Based,Human Error","10.38","Medium","","","No:-1 engine room vent fan junction box contain little moisture inside it. So box opened up and made it as water tight and 440v resistance reached infinity.","2021-04-16T23:59:35","","Completed","2021-04-15T23:59:35","No","No","No","Internal"]
[null,null,null,19505,null,"45_03/05/2021 20:27:50","2021-04-09T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Emergency Generator 220V feeder circuit resistance less than infinity","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Behaviour Based,Human Error","10.38","Medium","","","Light casing outside the Paint locker contain little moisture inside it, casing renewed and resistance increased to infinity.","2021-04-16T23:59:35","","Completed","2021-04-12T23:59:35","No","No","No","Internal"]
[null,null,null,19506,null,"45_03/05/2021 19:45:20","2021-04-09T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Accommodation front wall to spot de-rust & paint","Miscellaneous","General Appearance","External Factors","11.8","Low","","","Accomodation front wall Cleaned, Spot Derusted & Re-Painted","2021-07-08T23:59:35","","Completed","2021-05-01T23:59:35","No","No","No","Internal"]
[null,null,null,19507,null,"45_03/05/2021 19:56:00","2021-04-09T23:59:35","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Gym equipment to secure","Accommodation","General Appearance","External Factors","11.13","Low","","","Gym Equipment secured with Anti-Skid mats","2021-05-08T23:59:35","","Completed","2021-05-01T23:59:35","No","No","No","Internal"]
[null,null,null,19508,null,"45_03/05/2021 19:58:06","2021-04-09T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Paint drum over stacked, provide additional securing arrangement\n\n","Miscellaneous","General Appearance","Behaviour Based,Human Error","9.14","Medium","","","Additional securing arrangement fabricated & put in place; Paints are now safely stacked/ stored.","2021-05-08T23:59:35","","Completed","2021-05-02T23:59:35","No","No","No","Internal"]
[null,null,null,19509,null,"45_03/05/2021 19:49:12","2021-04-09T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Weather deck on top of Pump room to derust & paint","Miscellaneous","General Appearance","External Factors","11.8","Low","","","Weather deck on top of pumproom Derusting - Buffing followed by 2 coat Primer & Final top coat completed.","2021-05-08T23:59:35","","Completed","2021-05-06T23:59:35","No","No","No","Internal"]
[null,null,null,19510,null,"45_03/05/2021 20:31:07","2021-04-09T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Include SOX scrubber deck house smoke detectors in monthly report\n\n\n\n","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Inappropriate Procedure","5.35","Medium","","","SOX scrubber deck house Smoke detectors included in Monthly Report","2021-04-23T23:59:35","","Completed","2021-04-12T23:59:35","No","No","No","Internal"]
[null,null,null,19511,null,"45_03/05/2021 20:02:35","2021-04-09T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Main Deck electric cable support wasted at STBD side of value box 1A","Deck - Pipe / Fittings","General Appearance","External Factors","11.5","Medium","","","Main Deck electric cable support renewed & put back in place.","2021-05-08T23:59:35","","Completed","2021-05-08T23:59:35","No","No","No","Internal"]
[null,null,null,18982,null,"45_15/04/2021 7:17:01 PM","2021-04-14T23:59:35","Defect","Ship Staff","Ship Staff Insp.","AFT ETA storage box cabinet door hinges are broken.","Deck - Mooring Machinery,Miscellaneous","General Appearance","Equipment Related,External Factors","11.3","Medium","","","AFT ETA storage box cabinet door hinges renewed.","2021-04-20T23:59:35","","Completed","2021-04-18T23:59:35","No","No","No","Internal"]
[null,null,null,18981,null,"45_15/04/2021 7:49:52 PM","2021-04-15T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Port side Pumproom blower not Operational due to broken coupling in motor side.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","5.18","High","","","pump room coupling fabricated onboard and assembled in motor and tried out, currently it is working fine. intermediate coupling inspection carried out .Requisition raised, original spare received onboard and kept as spare.","2021-07-14T23:59:35","SCAN210081","Completed","2021-06-18T23:59:35","No","No","No","Internal"]
[null,null,null,19497,null,"45_14/05/2021 3:42:16 PM","2021-05-02T23:59:35","Defect","Ship Staff","Ship Staff Insp.","VALVE REMOTE CONTROL SYSTEM PUMP OUTLET PRESSURE GAUGE FAULTY","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Pressure gauge renewed with new pressure gauge","2021-06-30T23:59:35","SCAN210094","Completed","2021-06-10T23:59:35","No","No","No","Internal"]
[null,null,null,19496,null,"45_03/05/2021 19:28:32","2021-05-03T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Paint peel of on main deck at various isolated locations from midship to Foc'scle.","Miscellaneous","General Appearance","External Factors","11.1","High","","","Derusting/ Scrapping followed by 2 coats of primer & Spot Final Coat completed on Port Side main deck Fwd to midship.","2021-08-02T23:59:35","","Completed","2021-06-16T23:59:35","No","No","No","Internal"]
[null,null,null,19726,null,"45_15/06/2021 12:32:19 PM","2021-05-05T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Repeater panel MN400 on the bridge giving EXT alarm E1 WBT system fault.","Elect. Mach. & Equip.","Cargo / Ballast Systems","Equipment Related","10.32","Very High","","","Checked the system, repeater panel is common for both pump room gas alarm system and water ballast tank system. theres is no alarm in th main panel in CCR, all checks carried out as per technician advice. seems to be configuration error. Issue Rectified by shore technician @ Singapore 17 Aug 2021","2021-08-31T23:59:35","SCAN 215045","Completed","2021-08-17T23:59:35","No","No","No","Internal","Service engineer will be arranged inSingapore."]
[null,null,null,19498,null,"45_14/05/2021 9:21:25 PM","2021-05-06T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Maine engine unit no6 fuel pump leakage.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","changed with spare overhauled fuel pump","2021-07-31T23:59:35","","Completed","2021-06-30T23:59:35","No","No","No","Internal"]
[null,null,null,19499,null,"45_14/05/2021 11:27:17","2021-05-14T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Unable to start/ Run both WBP simultaneously for De-ballasting operation using BWTS system ","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","6.21","High","","","Defect Added in GC list.","2021-08-13T23:59:35","","Completed","2021-06-01T23:59:35","No","No","No","Internal"]
[null,null,null,19545,null,"45_31/05/2021 9:14:20 PM","2021-05-14T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Main engine fuel leak off alarm sensor malfunctioning. ","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Replaced with new spare.","2021-08-31T23:59:35","scan210074","Completed","2021-06-09T23:59:35","No","No","No","Internal"]
[null,null,null,19540,null,"45_30/05/2021 9:48:47 PM","2021-05-17T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","Fwd piston horn found not  working, same opened for inspection, piston and connecting rod in broken condition.","Navigation - Others","Communication","Equipment Related","12.12","High","","","overhauled with new spare.","2021-08-31T23:59:35","SCAN210075","Completed","2021-06-10T23:59:35","No","No","No","Internal"]
[null,null,null,19541,null,"45_30/05/2021 9:52:35 PM","2021-05-18T23:59:35","Defect","Ship Staff","Ship Staff Insp.","HYDROPHORE PUMP DISCHARGE NON RETURN VALVE DISC NOT CLOSING PROPERLY.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","New valve replaced.","2021-08-30T23:59:35","SCAN210095","Completed","2021-06-12T23:59:35","No","No","No","Internal"]
[null,null,null,19539,null,"45_28/05/2021 16:08:32","2021-05-20T23:59:35","Defect","Ship Staff","Ship Staff Insp.","During Routine Inspection of FPK WBT vent head, found vent float is broken.","Deck - Pipe / Fittings,Hull & Tanks","Structural Condn. / WT integrity ","Equipment Related","11.7","High","","","Renewed with new float.","2021-08-19T23:59:35","SCAN210100","Completed","2021-06-15T23:59:35","No","No","No","Internal"]
[null,null,null,19542,null,"45_30/05/2021 10:00:03 PM","2021-05-22T23:59:35","Defect","Ship Staff","Ship Staff Insp.","AFT PEAK TANK FCV3211 VALVE MALFUNCTIONING, NEED TECHNICIAN ASSISTANCE OR TO RENEW THE VALVE UNDER GURANTEE CLAIM","Miscellaneous","Cargo / Ballast Systems","Equipment Related","","","","","TECHNICIAN came onboared and rectified the faults.","2021-08-29T23:59:35","","Completed","2021-06-07T23:59:35","No","No","No","Internal"]
[null,null,null,19543,null,"45_30/05/2021 9:55:41 PM","2021-05-23T23:59:35","Defect","Ship Staff","Ship Staff Insp.","HFO PURIFIER CLEAN OIL OUTLET FLEXIBLE HOSE LEAKING.","E/R - Purifier","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","fexible hose renewed with new spare.","2021-09-30T23:59:35","SCAN210104","Completed","2021-09-04T23:59:35","No","No","No","Internal","Spares on order, will bee supplied once ready."]
[null,null,null,19544,null,"45_28/05/2021 16:16:29","2021-05-24T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Ballast tank level gauging - Level master H8   is giving frequent alarm/ Error; \"“BLOCKERR” LED illuminated","Miscellaneous","Cargo / Ballast Systems","Equipment Related","8.13","Medium","","","H8 Utility software CD installed and tried out, alarms start indicating in panel, still the problem persists. Rectified by Shore Technician @ Singapore on 17 Aug 2021.","2021-08-23T23:59:35","SCAN 215047","Completed","2021-08-17T23:59:35","No","No","No","Internal","send mail with present status."]
[null,null,null,19991,null,"45_18/06/2021 14:13:34","2021-06-07T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Fwd of manifold – main deck coating at various stages of paint peel off","Miscellaneous","General Appearance","External Factors","11.1","High","","","Derusting/ Buffing followed by 2 coat of primer & Spot Final coat painting completed.","2021-09-06T23:59:35","","Completed","2021-08-16T23:59:35","No","No","No","Internal","Please update progress on same with every DDRL."]
[null,null,null,19992,null,"45_27/6/2021 9:53:57 AM","2021-06-07T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Personal transfer basket - More than 7 years old – to raise RO for replacement","Miscellaneous","Safety / LSA / FFA","Inappropriate Procedure","5.47","Medium","","","New Personal Transfer Basket Procured & put in use,Old Personal transfer basket discarded from Use. Received new personal transfer basket @ Singapore 17 Aug 2021.","2021-09-06T23:59:35","SCAN 210118","Completed","2021-08-17T23:59:35","No","No","No","Internal","Spare on order, will be supplied at next call Singapore."]
[null,null,null,19993,null,"45_29/06/2021 12:20:12 AM","2021-06-07T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Fish room and meat room door handles broken – to procure new handle and replace","Miscellaneous","General Appearance","Equipment Related","11.17","Low","","","New hanlde changed.","2021-08-30T23:59:35","SCAN210127","Completed","2021-08-21T23:59:35","No","No","No","Internal"]
[null,null,null,19994,null,"45_18/06/2021 13:30:27","2021-06-07T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Ship Staff Insp.","Rudder angle indicator shows an error of 3 degree from local Auto pilot panel","Navigation - Others","Navigation","Equipment Related","10.41","Medium","","","Required to adjust from steering gear room informed to kamlesh solanki regarding this issue. Torque motor, control rod lever turn buckle adjusted. It was working fine for few days. Again the problem raised. will do the fine tuning and will update in next report.","2021-08-31T23:59:35","","Completed","2021-08-07T23:59:35","No","No","No","Internal","Target date revised, as need to adjust again."]
[null,null,null,19995,null,"45_18/06/2021 13:27:20","2021-06-07T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","EGCS tower room\tNatural vent wire mesh in various stages of corrosion","Miscellaneous","General Appearance","External Factors","11.7","High","","","EGCS tower room -\tNatural vent wire mesh & Flap Derusted followed by 1 Coat primer & Final coat Completed.","2021-06-26T23:59:35","","Completed","2021-06-26T23:59:35","No","No","No","Internal"]
[null,null,null,19996,null,"45_18/06/2021 14:11:13","2021-06-07T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Fire wire reel Seized and not turning – greasing points painted over","Deck - Mooring Machinery","Mooring","Behaviour Based,Human Error","9.14","Medium","","","Fwd & Aft Fire wire reel freed up, Grease nipples renewed & Lubricated.","2021-07-02T23:59:35","","Completed","2021-06-19T23:59:35","No","No","No","Internal"]
[null,null,null,19997,null,"45_29/06/2021 12:23:35 AM","2021-06-07T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Damper near Top up air compressor – seized, not able to operate by remote leverOn ","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","damper removed from duct, derusted, eased up, painted, lubricated and boxed up.","2021-06-30T23:59:35","","Completed","2021-06-12T23:59:35","No","No","No","Internal"]
[null,null,null,19998,null,"45_18/06/2021 14:07:48","2021-06-07T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ER vent fans Housing – rust weepings and filter frames rusted","Miscellaneous","General Appearance","External Factors","11.7","High","","","ER vent fans Housing  - Derusting/ buffing  followed by 2 coat primer & Full final coat painting completed.","2021-07-06T23:59:35","","Completed","2021-06-22T23:59:35","No","No","No","Internal"]
[null,null,null,20077,null,"45_15/07/2021 3:11:15 PM","2021-07-06T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Main engine unit 6 fuel pump barrel sealing ring leaking.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Main engine unit 6 fuel pump changed with spare fuel pump. ","2021-09-30T23:59:35","","Completed","2021-08-30T23:59:35","No","No","No","Internal","Noted awaiting next opportunity."]
[null,null,null,20076,null,"45_15/07/2021 3:24:45 PM","2021-07-07T23:59:35","Defect","Ship Staff","Ship Staff Insp.","COPT no 3 auto grease cup is having crack.","Cargo Mach.","Eng. / Strg. Comp.","Equipment Related","8.8","Medium","","","renewed with new spare","2021-10-15T23:59:35","SCAN210140","Completed","2021-10-08T23:59:35","No","No","No","Internal","Spares on order and will be arranged at next available opportunity. Target date revised accordingly."]
[null,null,null,20078,null,"45_15/07/2021 3:16:05 PM","2021-07-10T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Bilge pump priming unit, auto valve bellow leaking.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Bilge pump priming unit auto valve  renewed.","2021-10-31T23:59:35","SCAN210139","Completed","2021-11-01T23:59:35","No","No","No","Internal","Spares will be arranged once ready. Understand pump is operational now. Target date revised."]
[null,null,null,20079,null,"45_15/07/2021 3:39:24 PM","2021-07-10T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Hot water calorifier steam controller is malfunctioning.","Accommodation,Miscellaneous","MLC Related","Equipment Related","10.32","Very High","","","Renewed with new spare","2021-10-15T23:59:35","SCAN210141","Completed","2021-10-08T23:59:35","No","No","No","Internal","Spares on order and will be connected at next opportunity.\nTarget date revised accordingly."]
[null,null,null,20223,null,"45_31/07/2021 3:45:31 PM","2021-07-20T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Steering gear system forward port ram seal is leaking and all there steering pumps are dragging during emcy manual steering mode.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Technician came onboard, changed the seal for no:-2 ram port fwd and dragging issue sorted out.","2021-10-31T23:59:35","","Completed","2021-08-17T23:59:35","No","No","No","Internal"]
[null,null,null,20385,null,"45_15/08/2021 9:19:43 PM","2021-08-12T23:59:35","Observation","Ship Staff","Ship Staff Insp.","OXYGEN/ACETYLENE hose connection secured with jublie clips. it need to be secured with ear clamps.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","oxy/acetelyne hose secured with ear clamp","2021-11-25T23:59:35","SCAN210172","Completed","2021-08-20T23:59:35","No","No","No","Internal"]
[null,null,null,20386,null,"45_15/08/2021 9:12:43 PM","2021-08-13T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Main engine local manouvering engine telegraph system, new command couldn't able to accept and internal failure alarm persist. After tapping the control box, internal failure alarm disappear.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Local manouvering panel card renewed with new spare.","2021-11-25T23:59:35","","Completed","2021-08-26T23:59:35","No","No","No","Internal","Spares will be supplied in Singapore."]
[null,null,null,20820,null,"45_15/09/2021 9:33:18 PM","2021-08-14T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Air condition plant NO:-2 compressor MCCB short circuited.","E/R - Aux. Mach.,Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","renewed with new spare.","2021-12-30T23:59:35","SCAN210189","Completed","2021-10-10T23:59:35","No","No","No","Internal"]
[null,null,null,20664,null,"45_27/08/2021 16:20:13","2021-08-17T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Exhaust pipes on funnel to be derusted and painted at available opportunity","E/R - Pipes/ valves & fittings","General Appearance","External Factors","11.1","High","","","Scrapping, Cleaning followed by painting of Exhaust pipes on funnel carried out.","2021-11-16T23:59:35","","Completed","2021-09-07T23:59:35","No","No","No","Internal"]
[null,null,null,20665,null,"45_27/08/2021 16:04:46","2021-08-17T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Port & Stbd windlass anchor hydraulic brake is set wrongly.","Deck - Mooring Machinery","Mooring","Equipment Related","9.14","Medium","","","brake adjusted and matched wih the indicator and tried out, found satisfactory.","2021-11-16T23:59:35","","Completed","2021-09-24T23:59:35","No","No","No","Internal"]
[null,null,null,20666,null,"45_27/08/2021 16:12:37","2021-08-17T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Two of the gratings at port side manifold needs to renew. Other needs to derust and paint.","Deck - Pipe / Fittings","General Appearance","External Factors","11.1","High","","","2 gratings at port  side cargo manifold drip tray renewed, Derusting/ painting of Port manifold drip tray grating & drip tray completed. ","2021-09-06T23:59:35","","Completed","2021-09-03T23:59:35","No","No","No","Internal"]
[null,null,null,20667,null,"45_27/08/2021 16:14:40","2021-08-17T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Both pump room blower casing to derust and paint.","Deck - Pipe / Fittings","General Appearance","External Factors","11.1","High","","","Derusting / buffing followed by  Painting & highlighting of Port & Stbd pumproom blower casing completed.","2021-11-16T23:59:35","","Completed","2021-09-09T23:59:35","No","No","No","Internal"]
[null,null,null,20668,null,"45_31/08/2021 11:42:37 AM","2021-08-17T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Stbd line ME lube oil bunker pipe line has pin hole. ","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","Equipment Related","11.4","Very High","","","Defective section renewed with new pipe section.","2021-09-20T23:59:35","","Completed","2021-09-07T23:59:35","No","No","No","Internal"]
[null,null,null,20669,null,"45_31/08/2021 11:47:58 AM","2021-08-17T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Rusted and wasted material of Rain protector for port side funnel door at E/R blower platform ","Miscellaneous","Structural Condn. / WT integrity ","Equipment Related","11.8","Low","","","defective area renewed with new plates.","2021-09-20T23:59:35","","Completed","2021-09-07T23:59:35","No","No","No","Internal"]
[null,null,null,20670,null,"45_31/08/2021 11:59:42 AM","2021-08-17T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Water in oil sensor is suspected to be defective. to check and rectify.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","water in oil sensor replaced with new spare, present reading 0.14 locally ,now working in good order","2021-11-30T23:59:35","SCAN210178","Completed","2021-11-08T23:59:35","No","No","No","Internal","Spares already supplied. Install at next port. Target date revised."]
[null,null,null,17855,null,"45_16/02/2021 1:03:54 PM","2021-08-17T23:59:35","Defect","Ship Staff","Ship Staff Insp.","M/E viscosity steam auto control valve malfunctioning, valve need to overhaul.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","valve gear parts opened and inspected again all were in good order,cams for the limitswitches re adjusted,one of the limit switches was showing open circuit same repaired by re soldering,valve tried out by varing the viscocity from the controller in the ECR and operation was found to be satisfactory.","2021-11-30T23:59:35","","Completed","2021-11-09T23:59:35","No","No","No","Internal","What is RO no for this?"]
[null,null,null,20671,null,"45_31/08/2021 12:02:35 PM","2021-08-17T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Both air con controller is very old and worn condition.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","11.1","High","","","NO:-1 and 2 AC compressor panel  controller card renewed.","2021-11-30T23:59:35","SCAN215059","Completed","2021-11-10T23:59:35","No","No","No","Internal","On order. Will be supplied once ready. Target date revised."]
[null,null,null,20672,null,"45_31/08/2021 12:08:40 PM","2021-08-17T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","CCTV onboard is not yet commisioned.","Miscellaneous","Communication","Equipment Related","11.1","High","","","installation completed","2021-10-31T23:59:35","","Completed","2021-09-08T23:59:35","No","No","No","Internal"]
[null,null,null,20673,null,"45_31/08/2021 1:09:22 PM","2021-08-17T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","BWTS panel near calorifier is not secured properly. ","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","6.21","High","","","frames fabricated and welded to the BWTS panel.","2021-09-20T23:59:35","","Completed","2021-09-03T23:59:35","No","No","No","Internal"]
[null,null,null,20674,null,"45_27/08/2021 16:07:44","2021-08-17T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Oil level in windlass gear case is not visible. To top up.","Deck - Mooring Machinery","Mooring","External Factors","9.14","Medium","","","Gear oil Renewed for P & S windlass gear case.","2021-08-24T23:59:35","","Completed","2021-08-24T23:59:35","No","No","No","Internal"]
[null,null,null,20675,null,"45_27/08/2021 16:17:47","2021-08-17T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Rust weep marks below the cable tray on main deck. To be attended","Deck - Pipe / Fittings","General Appearance","External Factors","11.1","High","","","Derusting / buffing followed by painting carried out at the rust weep marks. ","2021-09-30T23:59:35","","Completed","2021-08-30T23:59:35","No","No","No","Internal"]
[null,null,null,20676,null,"45_31/08/2021 11:24:27 AM","2021-08-17T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","EGCS ventilation louver to be fitted with wheel and to ease up.","Miscellaneous","ISM Related","Equipment Related","10.32","Very High","","","Wheel fabricated and operating hanle interchanged with wheel. After changing the hand wheel, flaps ease up.","2021-08-31T23:59:35","","Completed","2021-08-27T23:59:35","No","No","No","Internal"]
[null,null,null,20677,null,"45_31/08/2021 11:53:42 AM","2021-08-17T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Some bunker pipelines at break of accomodation are marked with paint marker. same to be stenciled.","Deck - Pipe / Fittings","General Appearance","Human Error","11.4","Very High","","","stencil work  carried out for bunker pipeline at break of accomodation.","2021-08-27T23:59:35","","Completed","2021-08-24T23:59:35","No","No","No","Internal"]
[null,null,null,20678,null,"45_31/08/2021 12:18:31 PM","2021-08-17T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Steering gear pump need to paint.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.43","Medium","","","Steering gear pump painting work carried out.","2021-09-17T23:59:35","","Completed","2021-08-26T23:59:35","No","No","No","Internal"]
[null,null,null,20679,null,"45_31/08/2021 12:34:49 PM","2021-08-17T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Stbd DG FO filter lagging to renew.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.19","Very High","","","Stbd DG  FO filter lagging fixed properly and additional lagging used.","2021-08-24T23:59:35","","Completed","2021-08-22T23:59:35","No","No","No","Internal"]
[null,null,null,20680,null,"45_31/08/2021 12:40:47 PM","2021-08-17T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Atmospheric drain valve wheel and cap missing.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Spare wheel and cap fixed in valve.","2021-08-24T23:59:35","","Completed","2021-08-21T23:59:35","No","No","No","Internal"]
[null,null,null,20681,null,"45_31/08/2021 12:51:29 PM","2021-08-17T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ME liner tool is lying unsecured.","Miscellaneous","General Appearance","Human Error","10.29","Medium","","","ME liner tool secured.","2021-08-24T23:59:35","","Completed","2021-08-21T23:59:35","No","No","No","Internal"]
[null,null,null,20682,null,"45_31/08/2021 12:58:36 PM","2021-08-17T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Various weather tight doors of EGCS room and entrance to engine room does not have open close marking","Miscellaneous","General Appearance","Behaviour Based,Human Error","11.4","Very High","","","Open, shut marking painted in EGCS doors","2021-08-24T23:59:35","","Completed","2021-08-19T23:59:35","No","No","No","Internal"]
[null,null,null,20683,null,"45_31/08/2021 1:06:59 PM","2021-08-17T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Old and removed main air compressor body to shift to safe location.","E/R - Air Comp.","General Appearance","Equipment Related","10.29","Medium","","","Old and removed main air compressor body shifted to safe location top of ECR.","2021-08-30T23:59:35","","Completed","2021-08-22T23:59:35","No","No","No","Internal"]
[null,null,null,20684,null,"45_31/08/2021 1:11:47 PM","2021-08-17T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ME Air cooler U-tube manometer is empty.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Liquid filled up in U-tube manometer","2021-08-24T23:59:35","","Completed","2021-08-22T23:59:35","No","No","No","Internal"]
[null,null,null,20821,null,"45_15/09/2021 9:26:54 PM","2021-09-06T23:59:35","Defect","Ship Staff","Ship Staff Insp.","NO:-2 HFO purifier water block is faulty and purifier is not in use.","E/R - Purifier","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","water block replaced with new spare.","2021-12-26T23:59:35","","Completed","2021-12-13T23:59:35","No","No","No","Internal","Awaiting Readiness"]
[null,null,null,20822,null,"45_15/09/2021 9:44:18 PM","2021-09-09T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Vacuum toilet system vaccum control mechanism for few cabin toilets and engine room toilet found malfunctioning.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Required to renew the control mechanism, RO raised to keep some in spare.","2021-12-31T23:59:35","SCAN210188","Completed","2021-09-11T23:59:35","No","No","No","Internal"]
[null,null,null,20823,null,"45_15/09/2021 9:48:33 PM","2021-09-11T23:59:35","Observation","Ship Staff","Ship Staff Insp.","IG inlet valve to scrubber, 5/2 way direction control valve found leaking. ","E/R - Pipes/ valves & fittings,Inert Gas","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","5/2 way valve opened and inspected, telfon seals got damaged. required to renew the valve. RO raised.","2021-12-29T23:59:35","SCAN210173","Completed","2021-10-12T23:59:35","No","No","No","Internal"]
[null,null,null,20824,null,"45_15/09/2021 9:41:22 PM","2021-09-13T23:59:35","Defect","Ship Staff","Ship Staff Insp.","ME fuel oil auto back wash filter. diversion filter element found damaged during maintenance. spacer found crack near the stud securing slot.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Spacer renewed with new spare, for diversion filter element RO raised for same to keep in spare.","2021-12-28T23:59:35","SCAN210187","Completed","2021-09-14T23:59:35","No","No","No","Internal"]
[null,null,null,20825,null,"45_15/09/2021 9:37:27 PM","2021-09-15T23:59:35","Defect","Ship Staff","Ship Staff Insp.","In Engine control room NO:-2 440V feeder panel Air condition plant no:-2 compressor circuit breaker short circuited.","E/R - Aux. Mach.,Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","shunt coil taken from old breaker and fitted .Tested the Prefential trips  and found it in good working condition.","2021-12-31T23:59:35","SCAN210189","Completed","2021-11-20T23:59:35","No","No","No","Internal","Spare On order."]
[null,null,null,21290,null,"45_26/9/2021 8:52:18 PM","2021-09-26T23:59:35","Defect","Ship Staff","Ship Staff Insp.","NO # 2 Purifier friction pad parallel pin renewal for the motor drive unit.","E/R - Purifier","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","damaged friction pad parallel pin threads re dressed and tightened with thread lock.New Clutch drum received and renewed.Purifier tested,satisfactory.Put in operation","2022-02-28T23:59:35","SCAN210212","Completed","2022-03-08T23:59:35","No","No","No","Internal",""]
[null,null,null,20819,null,"45_15/09/2021 9:29:58 PM","2021-10-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","A/E 1,2,3 jacket water high temperature thermostat found malfunctioning. operation of thermostat is eratic.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Thermostat renewed, working satisfactory.","2022-01-31T23:59:35","","Completed","2022-01-29T23:59:35","No","No","No","Internal","readiness is end Nov."]
[null,null,null,21620,null,"45_13/10/2021 14:48:31","2021-10-05T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","No 7 foam monitor found leaking from flange.","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.35","Medium","","","No 7 foam monitor was removed from position,  cold work was done on the face of the leaking flange then smoothened . Same tested and no leaks observed .","2021-11-30T23:59:35","","Completed","2021-11-05T23:59:35","No","No","No","Internal","To be attended on priority basis"]
[null,null,null,21621,null,"45_14/10/2021 11:13:23 AM","2021-10-05T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","IGG panel to renew","E/R - Aux. Mach.,Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Panel renewed with new spare and IGG fired and tested all was found in good order O2 3.6 recorded .","2021-11-25T23:59:35","","Completed","2021-10-15T23:59:35","No","No","No","Internal"]
[null,null,null,21622,null,"45_14/10/2021 11:17:42 AM","2021-10-05T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","The air duct above ME to clean and paint.","Miscellaneous","Eng. / Strg. Comp.","External Factors","11.13","Low","","","Cleaning and painting carried out.","2022-01-30T23:59:35","","Completed","2022-01-07T23:59:35","No","No","No","Internal","Target date revised as work is in progress."]
[null,null,null,21623,null,"45_14/10/2021 11:22:11 AM","2021-10-05T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Sewage treatment plant blower casing is damaged, need to renew.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Repair work carried out.Now all in good order.","2022-01-19T23:59:35","SCAN210131","Completed","2021-12-22T23:59:35","No","No","No","Internal"]
[null,null,null,21624,null,"45_14/10/2021 11:44:00 AM","2021-10-05T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ODME spare as recommended by service engineer to renew.","Miscellaneous","MARPOL Related","Equipment Related","6.14","High","","","The zener barrier and the pressure switch has been replaced and ODME tried out in simulation mode and all found in good order.  ","2021-12-15T23:59:35","","Completed","2021-10-16T23:59:35","No","No","No","Internal"]
[null,null,null,21625,null,"45_14/10/2021 11:48:53 AM","2021-10-05T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","The vent head of hotwell in china passage to clean and painty","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.6","Medium","","","The vent head of hotwell cleaned and painted","2022-01-31T23:59:35","","Completed","2022-01-17T23:59:35","No","No","No","Internal","Now vessel is in port. Complete tit."]
[null,null,null,21626,null,"45_14/10/2021 11:51:30 AM","2021-10-05T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Elevator door closure motor is making noise and bearing need to renew.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Elevator cage door closing motor overhauled, bearings replaced with new spare.","2021-11-11T23:59:35","","Completed","2021-10-19T23:59:35","No","No","No","Internal"]
[null,null,null,21628,null,"45_13/10/2021 14:53:55","2021-10-05T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Lowering handle of Stbd lifeboat is thinned down at one location. To repair.","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.29","High","","","Lowering handle of Stbd lifeboat repaired.","2021-10-14T23:59:35","","Completed","2021-10-13T23:59:35","No","No","No","Internal"]
[null,null,null,21629,null,"45_13/10/2021 15:21:24","2021-10-05T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Crew smoke room carpet to clean","Accommodation","General Appearance","External Factors","11.13","Low","","","Cleaning of Crew smoke room carpet carried out.","2021-10-21T23:59:35","","Completed","2021-10-15T23:59:35","No","No","No","Internal"]
[null,null,null,21630,null,"45_13/10/2021 15:15:13","2021-10-05T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Antiskid mat to lay on both bridge wing.","Miscellaneous","General Appearance","Behaviour Based","5.47","Medium","","","Antiskid Rubber mats put in place at both bridge wings.","2021-10-19T23:59:35","","Completed","2021-10-13T23:59:35","No","No","No","Internal"]
[null,null,null,21627,null,"45_14/10/2021 12:01:47 PM","2021-10-10T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Fresh water tank level gauge is not working properly.","Elect. Mach. & Equip.,Hull & Tanks","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Sensor renewewd, level gauge working satisfactory","2022-02-28T23:59:35","SCAN210217","Completed","2022-02-14T23:59:35","No","No","No","Internal","Yet to get quotation"]
[null,null,null,22268,null,"45_19/10/2021 20:09:54","2021-10-19T23:59:35","Observation","Ship Staff","Ship Staff Insp.","6 Number of Loose stud found on stbd anchor chain; Namely between kenter joining shackle 5 & 4 – 4 studs; between kenter joining shackle 3 & 2 – 2 studs","Deck - Mooring Machinery","Mooring","Equipment Related","9.21","Medium","","","Loose stud to be welded in place after getting concurrence for hotwork from office. The job has been deferred to drydock and the same has been updated in REFMAN for \"DEFECTS TO OFFICE 2021\"","2022-01-18T23:59:35","","Completed","2021-11-30T23:59:35","Yes","No","No","Internal"]
[null,null,null,22269,null,"45_01/11/2021 10:52:33 AM","2021-10-31T23:59:35","Defect","Ship Staff","Ship Staff Insp.","ME  main control air line pipe leakage as crak was noticed at the pipe  weld seam area.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","External Factors","10.32","Very High","","","Leak rectified by doing hot work.","2021-11-25T23:59:35","SCAN210187","Completed","2021-11-04T23:59:35","No","No","No","Internal","Attend on priority basis."]
[null,null,null,22270,null,"45_01/11/2021 23:45:56","2021-10-31T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Sea water inlet pipe for deck seal, on deck found to be heavily corroded. Need to renew.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.27","Medium","","","The corroded section of pipe was replaced with the newly fabricated pipe","2021-12-30T23:59:35","","Completed","2021-11-19T23:59:35","No","No","No","Internal","Attend this on priority basis."]
[null,null,null,22567,null,"45_16/11/2021 3:31:13","2021-11-02T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Seawater supply to deck seal pipe on deck found to fully wasted, new pipe to be fabricated and replaced","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.27","Medium","","","The corroded section of pipe was replaced with the newly fabricated pipe","2021-12-31T23:59:35","","Completed","2021-11-19T23:59:35","No","No","No","Internal","Plan for same at the first opportunity."]
[null,null,null,22568,null,"45_16/11/2021 3:35:47","2021-11-02T23:59:35","Observation","Ship Staff","Ship Staff Insp.","IG to ballast line on deck found to have a soft patch, temporary repair found using plug and devcon","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.3","Very High","","","The complete length of pipe to be fabricated in drydock. The job has been added in REFMAN with all the details and photos","2022-02-01T23:59:35","","Completed","2022-01-17T23:59:35","Yes","No","No","Internal","To be planned at available opportunity.  Understand material is available."]
[null,null,null,23170,null,"45_20/12/2021 1:56:53 PM","2021-12-15T23:59:35","Non Conformity","Ship Staff","Ship Staff Insp.","THE IG MAIN LINE  LOW PRESSURE SWITCH FAULTY.","Inert Gas","Cargo / Ballast Systems","Equipment Related","10.32","Very High","","","PRESSURE SWITCH RENEWED WITH NEW SPARE RECEIVED","2022-01-30T23:59:35","","Completed","2022-01-14T23:59:35","No","No","No","Internal"]
[null,null,null,23294,null,"45_03/01/2022 21:33:07","2021-12-18T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Mooring winch hydraulic return line developed a hole, due to wastage of metal.","Deck - Mooring Machinery","Mooring","Equipment Related","9.14","Medium","","","The holed section of pipe was removed, new pipe fabricated and fitted back. Purging of the system carried out. Winch tested, no leaks observed.","2022-01-31T23:59:35","","Completed","2022-01-28T23:59:35","No","No","No","Internal"]
[null,null,null,23293,null,"45_3/01/2022 8:47:16 AM","2021-12-19T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","No #3 E/R fan Damper flap top half broke and fell on the fan impeller causing severe damage/pulverization of the impeller and resulted in breakage of the motor foundation.","Deck - Pipe / Fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Shore technician replaced the old damper and motor with new, counterweight and pneumatic levers welded onboard to shaft, now working satisfactory","2022-01-31T23:59:35","SCAN215083 .MOTOR REQ WILL BE MADE OFFICE SIDE","Completed","2022-01-11T23:59:35","No","No","No","Internal"]
[null,null,null,23295,null,"45_3/01/2022 9:04:55 AM","2021-12-20T23:59:35","Defect","Ship Staff","Ship Staff Insp.","INCINERATOR GARBAGE DOSING SIGHT GLASS BROKEN, AND THE SOLENOID VALVE FOR OPENING THE SLUICE DOOR LEAKING","Critical Equip.,Elect. Mach. & Equip.","MARPOL Related","Equipment Related","10.32","Very High","","","SOLENOID VALVE RECEIVED AND SAME RENEWED, TRIED OUT, WORKING SATISFACTORY","2022-01-30T23:59:35","SCAN210257","Completed","2022-01-11T23:59:35","No","No","No","Internal"]
[null,null,null,23296,null,"45_3/01/2022 8:53:24 AM","2021-12-28T23:59:35","Other","Ship Staff","Ship Staff Insp.","DG PRE HEATER CONTROLLER FAULTY","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","THE HEATER CONTROLLER REPLACED WITH NEW SPARE WORKING SATISFACTORY","2022-02-28T23:59:35","SCAN220007","Completed","2022-03-05T23:59:35","No","No","No","Internal"]
[null,null,null,23298,null,"45_3/01/2022 9:14:14 AM","2022-01-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","THE EGCS WASH WATER EFFLUENT ANALYZER SC1000 UNIT OUTPUT CARD IS DEFECTIVE.","Critical Equip.","MARPOL Related","Equipment Related","10.32","Very High","","","THE HMI PANEL IN ECR READINGS SHOWS OVER LIMIT.BUT THE LOCAL READINGS ARE CORRECT.REQUISITION RAISED FOR THE SAME.NEW PCB RECEIVED AND INSTALLED,SATISFACTORY","2022-03-28T23:59:35","SCAN220003","Completed","2022-04-09T23:59:35","No","No","No","Internal"]
[null,null,null,23299,null,"45_3/01/2022 9:17:59 AM","2022-01-03T23:59:35","Defect","Ship Staff","Ship Staff Insp.","AIR CON CONDENSER PIPING RUBBER VIBRATION DAMPER BELLOW  CONDITION HAS DETERIORATED, HAVE HEAT CRACKS.","E/R - Pipes/ valves & fittings,Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","HAVE TO BE REPLACED SPARE ON ORDER.RUBBER EXPANSION BELLOW RENEWED","2022-03-28T23:59:35","SCAN220008","Completed","2022-04-12T23:59:35","No","No","No","Internal"]
[null,null,null,23300,null,"45_3/01/2022 9:23:46 AM","2022-01-03T23:59:35","Defect","Ship Staff","Ship Staff Insp.","AUX BOILER NO #2 FEED WATER CONTROLLER FOR HIGH MODE OPERATION POSITIONER FAULTY LEVEL NOT MAINTAINING IN AUTO MODE","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","POSITIONER RECALIBRATED, NOW FOUND TO BE WORKING SATISFACTORY, NEW POSITIONER RECEIVED KEPT AS SPARE","2022-01-31T23:59:35","SCAN220004","Completed","2022-01-10T23:59:35","No","No","No","Internal"]
[null,null,null,23539,null,"45_15/01/2022 2:58:15 PM","2022-01-09T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Boiler main panel handle is missing","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Handles fixed back","2022-03-09T23:59:35","","Completed","2022-01-20T23:59:35","No","No","No","Internal"]
[null,null,null,23540,null,"45_15/01/2022 3:04:54 PM","2022-01-09T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Atmospheric condenser sea water inlet pipe one section is temporarily repaired","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","New section fabricated and fixed back","2022-02-15T23:59:35","","Completed","2022-01-20T23:59:35","No","No","No","Internal"]
[null,null,null,23542,null,"45_15/01/2022 3:29:42 PM","2022-01-09T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Paint of bulkhead near stbd boiler burner top found in cracked condition due to high temp od sludge holding tank","Miscellaneous","Eng. / Strg. Comp.","External Factors","10.32","Very High","","","Old paint scrapped, cleaned and repainted","2022-01-31T23:59:35","","Completed","2022-01-22T23:59:35","No","No","No","Internal"]
[null,null,null,23543,null,"45_15/01/2022 3:50:48 PM","2022-01-09T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Incinerator milling pump found with leak marks","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Marks cleaned, painted and lagging renewed","2022-01-31T23:59:35","","Completed","2022-01-15T23:59:35","No","No","No","Internal"]
[null,null,null,23544,null,"45_15/01/2022 3:58:38 PM","2022-01-09T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Stbd boiler main steam stop valve leaking from gland","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Leak repaired by replacing with new gland","2022-02-09T23:59:35","","Completed","2022-01-22T23:59:35","No","No","No","Internal"]
[null,null,null,23545,null,"45_15/01/2022 4:00:52 PM","2022-01-09T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","OIl found collected in ME recess well","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.2","Low","","","Leak source to be identified, area to be cleaned.ME endcover bolts tightness checked and tightened.Area cleaned","2022-03-30T23:59:35","","Completed","2022-03-20T23:59:35","No","No","No","Internal"]
[null,null,null,23547,null,"45_15/01/2022 19:08:54","2022-01-09T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Various grating at manifold are holed and needs to be renewed.","Miscellaneous","General Appearance","Equipment Related","6.6","Medium","","","The gratings on both the manifolds were renewed with the newly received fiber gratings. Same secured with the locking arrangement.","2022-01-29T23:59:35","","Completed","2022-01-29T23:59:35","No","No","No","Internal"]
[null,null,null,23548,null,"45_15/01/2022 19:12:17","2022-01-09T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","The conduit pipe for cable of Stbd midship  mast light to be renewed as same is badly corroded.","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.4","Very High","","","Conduit pipe de-rusted & painted. ","2022-03-28T23:59:35","","Completed","2022-03-25T23:59:35","No","No","No","Internal"]
[null,null,null,23549,null,"45_15/01/2022 3:17:35 PM","2022-01-09T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","FWG ejector pump stop switch damaged","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Switch renewed","2022-01-15T23:59:35","","Completed","2022-01-12T23:59:35","No","No","No","Internal"]
[null,null,null,23550,null,"45_15/01/2022 3:22:06 PM","2022-01-09T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Aux engine oil max filters not in operation","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","OIl max filters put in  operation","2022-01-09T23:59:35","","Completed","2022-01-09T23:59:35","No","No","No","Internal"]
[null,null,null,23551,null,"45_15/01/2022 3:55:30 PM","2022-01-09T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Light casing on engine room blower platform found filled with water","Elect. Mach. & Equip.","Structural Condn. / WT integrity ","Equipment Related","10.32","Very High","","","Water drained and cleaned, o- ring renewed","2022-01-14T23:59:35","","Completed","2022-01-14T23:59:35","No","No","No","Internal"]
[null,null,null,23781,null,"45_01/02/2022 4:46:55 PM","2022-01-22T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Pump room blower vibrations found to be abnormal under operation","Deck - Machinery","Cargo / Ballast Systems","Equipment Related","10.32","Very High","","","Blower casing found to be worn out, temorarily repaired by putting punch marks inside the casing.PO raised.VIBRATION FOUND REDUCED OVER PERIOD OF TIME.","2022-03-30T23:59:35","SCAN220018","Completed","2022-04-10T23:59:35","No","No","No","Internal"]
[null,null,null,23782,null,"45_31/01/2022 11:42:28","2022-01-26T23:59:35","Defect","Ship Staff","Ship Staff Insp.","During the routine maintenance on the stbd side provision crane, the oil gauge glass was observed to be leaking oil. Same opened up for inspection and found the gauge glass was broken.","Deck - Machinery","General Appearance","Equipment Related","8.5","Very High","","","New one received at singapore & replaced","2022-04-25T23:59:35","SCAN220017","Completed","2022-04-08T23:59:35","No","No","No","Internal"]
[null,null,null,23862,null,"45_14/02/2022 8:16:51 AM","2022-02-05T23:59:35","Observation","Ship Staff","Ship Staff Insp.","ME unit#2 and #6, VIT for fuel pumps found to be stuck","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","No.2 Unit VIT linkage eased up,under observation.No.6 unit lubricated,working well.","2022-03-31T23:59:35","","Completed","2022-03-07T23:59:35","No","No","No","Internal"]
[null,null,null,23864,null,"45_14/02/2022 8:24:03 AM","2022-02-10T23:59:35","Observation","Ship Staff","Ship Staff Insp.","LT temp found to be increasing during loaded voyage at 71  rpm","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","100 per LT coooler to be cleaned chemically, filter for same was cleaned before departure last port.Both LT filter chemical cleaning carried out.ME tested at 70.5 rpm with sea water temp 27 deg,temeperature was holding well at 36 deg c.","2022-03-31T23:59:35","","Completed","2022-03-13T23:59:35","No","No","No","Internal"]
[null,null,null,23865,null,"45_14/02/2022 8:42:29 AM","2022-02-11T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Stbd(Low) sea chest filter basket internal rubber coating found to be bulging.","E/R - Air Comp.,E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Rubber coating to be renewed, deferred to dry dock","2025-02-11T23:59:35","","Completed","2022-02-11T23:59:35","Yes","No","No","Internal"]
[null,null,null,23866,null,"45_14/02/2022 2:55:43 PM","2022-02-12T23:59:35","Defect","Ship Staff","Ship Staff Insp.","CO2 room fixed fire fighting extinguishing cabinet for pump room and engine room found to be broken","Critical Equip.","Safety / LSA / FFA","Equipment Related","5.4","High","","","Fabrication for temperory cabinet in progress, PO raised for new cabinets.Steel Cabinet fabricated and installed for pump room.E/R & P/R Cabinet renewed with new spare.","2022-03-31T23:59:35","SCAN220040","Completed","2022-04-13T23:59:35","No","No","No","Internal"]
[null,null,null,23868,null,"45_14/02/2022 2:22:16 PM","2022-02-13T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Shaft earthing device jubliee clip holding silver band found to be broken","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Jubilee clip renewed","2022-03-05T23:59:35","","Completed","2022-02-25T23:59:35","No","No","No","Internal"]
[null,null,null,23867,null,"45_15/02/2022 7:42:02 PM","2022-02-15T23:59:35","Defect","Ship Staff","Ship Staff Insp.","ER VENT FAN#4 MOTOR FOUND GIVING LOW INSULATION ALARM AND TRIPPED","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","MOTOR ISOLATED, INSULATION FOUND TO BE 0, MOTOR DISMANTLED AND CHECKED, FOUND TO BE BURNT, PO RAISED.NEW MOTOR RECEIVED AND FITTED IN PLACE.FAN ASSEMBLED AND TESTED,SATISFACTORY","2022-03-30T23:59:35","SCAN220047","Completed","2022-03-07T23:59:35","No","No","No","Internal","Motor will be supplied in Singapore."]
[null,null,null,24147,null,"45_21/02/2022 10:04:10","2022-02-21T23:59:35","Observation","Ship Staff","Ship Staff Insp.","The messenger rope & pick up rope for the Aft ETA was observed to be frayed, needs replacement.","Deck - Machinery","Safety / LSA / FFA","Equipment Related","9.28","Medium","","","RO - SCAN220026 raised for new messenger rope & pick up rope. Received at Singapore and the rope was replaced","2022-05-20T23:59:35","SCAN220026 ","Completed","2022-03-06T23:59:35","No","No","No","Internal"]
[null,null,null,24148,null,"45_01/03/2022 10:40:28 AM","2022-02-22T23:59:35","Observation","Ship Staff","Ship Staff Insp.","NO.2 Accomodation air conditioning unit performance found to be reduced","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","TEV(aft) renewed.Leak near disch valve rectified.AC put in use at 75% load.Under observation.AC put in use at 100%.Cabin temperature maintaining at 20-21 deg when ambient is 34 deg with sea water at 29 degc.","2022-03-10T23:59:35","","Completed","2022-03-04T23:59:35","No","No","No","Internal"]
[null,null,null,24149,null,"45_01/03/2022 10:59:15 AM","2022-02-23T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","Engine room vent fan motor#3, fell down in engine air duct casing during operation, causing fan and motor damage","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","New Motor recieved and fitted inplace after detailed investigations and RCA , PRE AND POST CHECKS CARRIED OUT AS REQUIRED ","2022-03-31T23:59:35",", WORKING SATISFACTORY","Completed","2022-03-11T23:59:35","No","No","No","Internal","Motor and fan will be supplied in Singapore."]
[null,null,null,24150,null,"45_02/03/2022 7:08:27 PM","2022-03-02T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Pin hole was found to be developed in OWS 3rd stage filter chamber casing","E/R - Aux. Mach.,Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Casing to be renewed.New spare casing replaced the damaged one.System tested,satisfactory","2022-03-20T23:59:35","","Completed","2022-03-24T23:59:35","No","No","No","Internal"]
[null,null,null,24320,null,"45_07/03/2022 14:42:49","2022-03-03T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Chain on the safety walkway on deck requires de-rusting","Miscellaneous","General Appearance","Equipment Related","11.8","Low","","","Walkway chain de-rusted & painted","2022-04-03T23:59:35","","Completed","2022-03-25T23:59:35","No","No","No","Internal"]
[null,null,null,24321,null,"45_07/03/2022 14:10:42","2022-03-03T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Power box for speaker phone on monkey island broken & tied with cable tie","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.16","Low","","","Permanent fixing of the power box.Defective JB renewed","2022-04-03T23:59:35","","Completed","2022-04-14T23:59:35","No","No","No","Internal"]
[null,null,null,24322,null,"45_07/03/2022 14:44:01","2022-03-03T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Focsle store requires to be arranged neatly","Accommodation","General Appearance","Behaviour Based","5.11","Low","","","F'clse store secured. Cleaned. Save all painted","2022-04-03T23:59:35","","Completed","2022-03-30T23:59:35","No","No","No","Internal"]
[null,null,null,24323,null,"45_07/03/2022 14:45:17","2022-03-03T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Oxygen room door latch is hanging","Accommodation","General Appearance","Equipment Related","11.5","Medium","","","Oxygen room door latch to be repaired.Latch repair completed","2022-04-03T23:59:35","","Completed","2022-03-26T23:59:35","No","No","No","Internal"]
[null,null,null,24324,null,"45_07/03/2022 14:49:18","2022-03-03T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Lifeboat davit requires proper greasing","LSA / FFA","Safety / LSA / FFA","Behaviour Based","5.28","Very High","","","Greasing of LB davit carried out","2022-04-03T23:59:35","","Completed","2022-03-27T23:59:35","No","No","No","Internal"]
[null,null,null,24325,null,"45_07/03/2022 14:53:05","2022-03-03T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Stbd side pilot ladder shifting winch not working effectively","Deck - Machinery","General Appearance","Equipment Related","5.47","Medium","","","Overhauedl the shifting winch motor for stbd side pilot ladder","2022-05-03T23:59:35","","Completed","2022-04-01T23:59:35","No","No","No","Internal"]
[null,null,null,24326,null,"45_07/03/2022 14:34:08","2022-03-03T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Ballast discharge pipe in PR to be painted","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","","","","","Ballast discharging elbow in PR painted after carrying of repair on the soft patch","2022-03-03T23:59:35","","Completed","2022-04-06T23:59:35","No","No","No","Internal"]
[null,null,null,24327,null,"45_06/03/2022 9:08:34","2022-03-03T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Nav Locker auto switch for light tied with cable tie.","Accommodation","Safety / LSA / FFA","Inappropriate Procedure","","","","","Removed the cable tie from limit switch","2022-04-03T23:59:35","","Completed","2022-03-05T23:59:35","No","No","No","Internal"]
[null,null,null,24328,null,"45_07/03/2022 14:39:39","2022-03-03T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Fresh water valve on main deck near 1C COT was found leaking","Deck - Pipe / Fittings","General Appearance","Equipment Related","","","","","Valve tightned & leak arrested","2022-04-03T23:59:35","","Completed","2022-03-05T23:59:35","No","No","No","Internal"]
[null,null,null,24329,null,"45_07/03/2022 14:27:28","2022-03-03T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Pin hole leak in BWTS filter drain pipe in PR","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","","","","","Leaking pipe removed to ER workshop & the section renewed","2022-04-03T23:59:35","","Completed","2022-03-10T23:59:35","No","No","No","Internal"]
[null,null,null,24330,null,"45_07/03/2022 14:20:38","2022-03-03T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Emergency light for lifeboat/ life raft rusted & not rotating properly","Deck - Pipe / Fittings","General Appearance","Equipment Related","","","","","De-rusting & painting of the same completed. The turn table is fully greased & moving freely","2022-04-03T23:59:35","","Completed","2022-03-10T23:59:35","No","No","No","Internal"]
[null,null,null,24331,null,"45_07/03/2022 14:19:00","2022-03-03T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Lifeboat fwd & aft gripes bottle screw corroded","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","De-rusting completed and painted","2022-04-03T23:59:35","","Completed","2022-03-10T23:59:35","No","No","No","Internal"]
[null,null,null,24332,null,"45_07/03/2022 14:13:43","2022-03-03T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Drain chocked on the accommodation on portside A-deck","Accommodation","General Appearance","Equipment Related","","","","","Chocking removed from the pipe by hammering externally","2022-04-03T23:59:35","","Completed","2022-03-04T23:59:35","No","No","No","Internal"]
[null,null,null,24333,null,"45_06/03/2022 9:15:34","2022-03-03T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Nav Locker garbage stored next to electrical items.","Accommodation","General Appearance","Inappropriate Procedure","","","","","Nav locker cleaned and arrnaged","2022-04-03T23:59:35","","Completed","2022-03-05T23:59:35","No","No","No","Internal"]
[null,null,null,24334,null,"45_07/03/2022 14:32:10","2022-03-03T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ODME line in PR found with oil stain near flange on lower platform","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","","","","","The flanges from where minor leak was observed were fully tightened. Oil stain on the flanges were cleaned & painted","2022-04-03T23:59:35","","Completed","2022-03-06T23:59:35","No","No","No","Internal"]
[null,null,null,24335,null,"45_07/03/2022 14:22:17","2022-03-03T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Lifeboat selflowering wire pulley shows signs of corrosion","LSA / FFA","General Appearance","Equipment Related","","","","","De-rusting & painting of the same completed","2022-04-03T23:59:35","","Completed","2022-03-10T23:59:35","No","No","No","Internal"]
[null,null,null,24336,null,"45_07/03/2022 14:47:40","2022-03-03T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Life boat embarkation ladder bottom rope is frading","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","Close up inspection of the rope carried out. Found in satisfactory condition","2022-04-03T23:59:35","","Completed","2022-03-12T23:59:35","No","No","No","Internal"]
[null,null,null,24337,null,"45_07/03/2022 14:36:03","2022-03-03T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Various lights in PR requires to be renewed","Elect. Mach. & Equip.","Safety / LSA / FFA","Equipment Related","","","","","Faulty lights in PR renewed","2022-04-03T23:59:35","","Completed","2022-03-08T23:59:35","No","No","No","Internal"]
[null,null,null,24338,null,"45_07/03/2022 14:25:43","2022-03-03T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Deck stores to be arranged","Accommodation","General Appearance","Behaviour Based","","","","","Deck store arranged & inventory taken","2022-04-03T23:59:35","","Completed","2022-03-11T23:59:35","No","No","No","Internal"]
[null,null,null,24339,null,"45_07/03/2022 14:24:05","2022-03-03T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Stencil on foam hose box amiss","LSA / FFA","Safety / LSA / FFA","Industry Issue","","","","","Foam hose box stencilling carried out","2022-04-03T23:59:35","","Completed","2022-03-14T23:59:35","No","No","No","Internal"]
[null,null,null,24340,null,"45_07/03/2022 14:15:57","2022-03-03T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Hinges for lifejacket safety box on portside LB deck broken. ","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","new hinge fitted for lifejacket box on portside LB deck","2022-04-03T23:59:35","","Completed","2022-03-13T23:59:35","No","No","No","Internal"]
[null,null,null,24341,null,"45_07/03/2022 14:51:26","2022-03-03T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Port lifeboat - Screw fitted on the engine cover is not secured","LSA / FFA","Safety / LSA / FFA","Behaviour Based","","","","","Screw tightned","2022-04-02T23:59:35","","Completed","2022-03-10T23:59:35","No","No","No","Internal"]
[null,null,null,24343,null,"45_07/03/2022 14:12:17","2022-03-03T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Stay wire for main mast to be inspected for condition","Accommodation","General Appearance","Equipment Related","","","","","Main mast stay wire inspected for condition. Greasing carried out. Wire is in good condition","2022-04-03T23:59:35","","Completed","2022-03-08T23:59:35","No","No","No","Internal"]
[null,null,null,24318,null,"45_07/03/2022 14:37:39","2022-03-03T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Mooring winch lever locking puns not in satisafactory condition","Deck - Mooring Machinery","Mooring","Equipment Related","9.15","Medium","","","MW pins de-rusted & painted","2022-04-03T23:59:35","","Completed","2022-03-26T23:59:35","No","No","No","Internal"]
[null,null,null,24342,null,"45_06/03/2022 9:18:11","2022-03-06T23:59:35","Breakdown,Observation","Ship Staff","Ship Staff Insp.","Pump room skylight cover hinges found broken.","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","Equipment Related","","","","","Remove the skylight cover to ER for permanent repair of hinges","2022-03-30T23:59:35","","Completed","2022-03-14T23:59:35","No","No","No","Internal"]
[null,null,null,24949,null,"45_03/04/2022 7:23:36 AM","2022-03-26T23:59:35","Defect","Ship Staff","Ship Staff Insp.","MAC NO.2 COUPLING RUBBER DAMAGED","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","WHILECHECKING FOR LOW INSULATION ISSUE ON MAC NO.2,OBSERVED RUBBERINSERT IN THE COUPLING DAMAGED.NEW COUPLING RUBBER RECEIVED AND REPLACED THE DEFECTIVE ONE.TESTED,SATISFACTORY","2022-04-07T23:59:35","220087","Completed","2022-04-14T23:59:35","No","No","No","Internal"]
[null,null,null,24950,null,"45_01/04/2022 12:08:23 PM","2022-03-30T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Egcs system ovbd fwd discharge line at bottom platform is having minor leak.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","office informed,leakage minimized and under observation, shore assistance arranged for anchorage at singapore.shore techncian attended vessel and replaced the defectiove section.EGCS tested while vsl was underway after singapore,satisfactory","2022-04-10T23:59:35","","Completed","2022-04-07T23:59:35","No","No","No","Internal"]
[null,null,null,24317,null,"45_06/03/2022 9:05:49","2022-03-03T08:00:00","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Suez Cabin wash basin drain line to be repaired","Accommodation","General Appearance","Equipment Related","11.13","Low","","","Old one replaced with new one","2022-05-03T08:00:00","DSCAN220065","Completed","2022-04-26T08:00:00","No","No","No","Internal"]
[null,null,null,23297,null,"45_3/01/2022 8:59:29 AM","2021-12-30T08:00:00","Defect","Ship Staff","Ship Staff Insp.","ME TOP BRACING NO #2 AIR LEAKGE FROM THE PRIMARY CHAMBER TO THE SECONDARY CHAMBERCAUSING THE POSITION PIN TO MOVE OUT.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","sPARES ON ORDER NEED TO BE OVERHAULED AND PRIMARY CHAMBER SEAL TO BE REPLACED .OTHER 3 TOP BRACINGS ARE IN GOOD ORDER.SPARES ON BOARD.TO BE TAKEN UP AT ANCHORAGE.CHECKED AND TOPPED UP WITH OIL.NEW PRESSURE GAUGE FITTED.THE INDICATOR IS IN NORMAL POSITIONWITH PRESSURE STEADY FOR MORE THAN 72 HOURS EXCEPT FOR MINOR SEEPAGE OF OIL.SO THIS DEFECT IS CLOSED.","2022-05-31T08:00:00","SCAN220002","Completed","2022-04-29T08:00:00","No","No","No","Internal"]

{"sheet":"Calc","index":2,"n_rows":28,"n_cols":12,"rows_kept":28,"cut":false,"hidden":true,"merged":[]}
["Def_type","Def_cause","Equipments","VIQrefno","Observer_code"]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,"Dim itemSele As Long"]
[null,null,null,null,null,null,null,null,null,null,null,"   dim startRow as integer"]
[null,null,null,null,null,null,null,null,null,null,null,"   startRow=1"]
[null,null,null,null,null,null,null,null,null,null,null,"        For itemSele = 0 To ListBox1.ListCount - 1"]
[null,null,null,null,null,null,null,null,null,null,null,"        If ListBox1.Selected(itemSele) = True Then"]
[null,null,null,null,null,null,null,null,null,null,null,"        Worksheets(\"WorksheetName\").Range(\"A\" & startRow).Value = ListBox1.List(itemSele)"]
[null,null,null,null,null,null,null,null,null,null,null,"        startRow = startRow + 1"]
[null,null,null,null,null,null,null,null,null,null,null,"        End If"]
[null,null,null,null,null,null,null,null,null,null,null,"        Next"]
[null,null,null,null,null,null,null,null,null,null,null,"Dim LastRowA As String"]
[null,null,null,null,null,null,null,null,null,null,null,"        Dim itemSele As Long"]
[null,null,null,null,null,null,null,null,null,null,null,"       Dim startRow as integer"]
[null,null,null,null,null,null,null,null,null,null,null,"        LastRowA = ActiveSheet.Cells(Rows.count, \"A\").End(xlUp).row"]
[null,null,null,null,null,null,null,null,null,null,null,"        startQue = 0"]
[null,null,null,null,null,null,null,null,null,null,null,"        For itemSele = 0 To ListBox1.ListCount - 1"]
[null,null,null,null,null,null,null,null,null,null,null,"        For startRow = 1 To LastRowA"]
[null,null,null,null,null,null,null,null,null,null,null,"        If Worksheets(\"WorksheetName\").Range(\"A\" & startRow).Value = ListBox1.List(itemSele) Then"]
[null,null,null,null,null,null,null,null,null,null,null,"        ListBox1.Selected(itemSele) = True"]
[null,null,null,null,null,null,null,null,null,null,null,"        Exit For"]
[null,null,null,null,null,null,null,null,null,null,null,"        End If"]
[null,null,null,null,null,null,null,null,null,null,null,"        Next j"]
[null,null,null,null,null,null,null,null,null,null,null,"        Next"]
[null,null,null,null,null,null,null,null,null,null,null,"        End If"]

{"sheet":"Areaofobs","index":3,"n_rows":17,"n_cols":2,"rows_kept":17,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Cargo / Ballast Systems",11]
["Cert. & Docu.",2]
["Communication",6]
["Crew Management",3]
["Emgcy. Systems",13]
["Eng. / Strg. Comp.",14]
["General Appearance",15]
["Ice Opns.",17]
["ISM Related",7]
["ISPS Related",10]
["MARPOL Related",9]
["MLC Related",4]
["Mooring",12]
["Navigation",5]
["Safety / LSA / FFA",8]
["Structural Condn. / WT integrity ",16]

{"sheet":"Vessel_type","index":4,"n_rows":1,"n_cols":2,"rows_kept":1,"cut":false,"hidden":true,"merged":[]}
["Vessel_type","ID"]

{"sheet":"Deficiency_type","index":5,"n_rows":8,"n_cols":3,"rows_kept":8,"cut":false,"hidden":true,"merged":[]}
["TITLE","Type of deficiency_description","ID"]
["Breakdown",null,6]
["Critical Equipment",null,4]
["Defect",null,1]
["Guarantee Claim",null,8]
["Non Conformity",null,2]
["Observation",null,3]
["Other",null,7]

{"sheet":"VIQrefno","index":6,"n_rows":427,"n_cols":3,"rows_kept":427,"cut":false,"hidden":true,"merged":[]}
["VIQ_ref_no","Risk Value of observation","ID"]
["1.1","Low",8243]
["1.10","Low",8252]
["1.11","Low",8253]
["1.12","Low",8254]
["1.13","Low",8255]
["1.14","Low",8256]
["1.15","Low",8257]
["1.16","Low",8259]
["1.17","Low",8260]
["1.18","Low",8261]
["1.19","Low",8262]
["1.2","Low",8244]
["1.20","Low",8263]
["1.21","Low",8265]
["1.22","Low",8266]
["1.23","Low",8267]
["1.24","Low",8268]
["1.25","Low",8269]
["1.26","Low",8270]
["1.3","Low",8245]
["1.4","Low",8246]
["1.5","Low",8247]
["1.6","Low",8248]
["1.7","Low",8249]
["1.8","Low",8250]
["1.9","Low",8251]
["1.99","High",11258]
["10.1","Medium",8461]
["10.10","High",8470]
["10.11","Medium",8471]
["10.12","Very High",8472]
["10.13","Very High",8473]
["10.14","Medium",8474]
["10.15","Low",8475]
["10.16","Very High",8476]
["10.17","Very High",8477]
["10.18","High",8478]
["10.19","Very High",8479]
["10.2","Low",8462]
["10.20","High",8480]
["10.21","Medium",8481]
["10.22","Low",8482]
["10.23","Medium",8483]
["10.24","Low",8484]
["10.25","Very High",8485]
["10.26","High",8486]
["10.27","Medium",8487]
["10.28","Low",8488]
["10.29","Medium",8489]
["10.3","Medium",8463]
["10.30","High",8490]
["10.31","Very High",8491]
["10.32","Very High",8492]
["10.33","High",8493]
["10.34","High",8494]
["10.35","Very High",8495]
["10.36","Very High",8496]
["10.37","Medium",8497]
["10.38","Medium",8498]
["10.39","High",8499]
["10.4","High",8464]
["10.40","Medium",8500]
["10.41","Medium",8501]
["10.42","Medium",8502]
["10.43","Medium",8503]
["10.44","Medium",8504]
["10.45","Very High",8505]
["10.46","High",8506]
["10.47","Medium",8507]
["10.48","High",8508]
["10.49","Medium",8509]
["10.5","Low",8465]
["10.50","High",8510]
["10.51","Low",8511]
["10.52","Medium",8512]
["10.53","Medium",8513]
["10.54","High",8514]
["10.55","Low",8515]
["10.6","Very High",8466]
["10.7","Medium",8467]
["10.8","Medium",8468]
["10.9","Medium",8469]
["10.99","High",8516]
["11.1","High",8420]
["11.10","Medium",8429]
["11.11","Very High",8430]
["11.12","Low",8431]
["11.13","Low",8432]
["11.14","Medium",8433]
["11.15","Low",8434]
["11.16","Low",8435]
["11.17","Low",8436]
["11.2","Medium",8421]
["11.3","Medium",8422]
["11.4","Very High",8423]
["11.5","Medium",8424]
["11.6","Medium",8425]
["11.7","High",8426]
["11.8","Low",8427]
["11.9","Low",8428]
["11.99","High",8437]
["12.1","High",8438]
["12.10","High",8448]
["12.11","High",8449]
["12.12","High",8450]
["12.13","High",8451]
["12.14","High",8452]
["12.15","High",8453]
["12.16","High",8454]
["12.17","High",8455]
["12.18","High",8456]
["12.19","High",8457]
["12.2","High",8439]
["12.20","High",8458]
["12.21","High",8459]
["12.3","High",8441]
["12.4","High",8442]
["12.5","High",8443]
["12.6","High",8444]
["12.7","High",8445]
["12.8","High",8446]
["12.9","High",8447]
["12.99","High",8460]
["2.1","Very High",8296]
["2.1.9","Very High",11259]
["2.10","Medium",8304]
["2.11","Medium",8305]
["2.12","Low",8306]
["2.13","Low",8307]
["2.14","Low",8308]
["2.15","Low",8309]
["2.16","Medium",8310]
["2.2","Medium",8297]
["2.3","High",8295]
["2.4","Medium",8298]
["2.5","Medium",8299]
["2.6","Low",8300]
["2.7","High",8301]
["2.8","High",8302]
["2.9","Medium",8303]
["2.99","High",8311]
["3.1","High",8312]
["3.2","Very High",8313]
["3.3","High",8314]
["3.4","Low",8294]
["3.5","Medium",8315]
["3.6","High",8316]
["3.7","Very High",8317]
["3.8","Very High",8318]
["3.99","High",8319]
["4.1","High",8320]
["4.10","High",8329]
["4.11","Medium",8330]
["4.12","Very High",8331]
["4.13","Very High",8332]
["4.14","Very High",8333]
["4.15","Very High",8334]
["4.16","Very High",8335]
["4.17","Very High",8336]
["4.18","Very High",8337]
["4.19","Low",8338]
["4.2","Medium",8321]
["4.20","Very High",8339]
["4.21","High",8340]
["4.22","Low",8341]
["4.23","High",8342]
["4.24","High",8343]
["4.25","Low",8344]
["4.26","Low",8345]
["4.27","High",8346]
["4.3","Medium",8322]
["4.4","High",8323]
["4.5","Very High",8324]
["4.6","Medium",8325]
["4.7","High",8326]
["4.8","Medium",8327]
["4.9","Medium",8328]
["4.99","High",8347]
["5.1","Very High",8517]
["5.10","High",8526]
["5.11","Low",8527]
["5.12","Medium",8528]
["5.13","High",8529]
["5.14","Very High",8530]
["5.15","Medium",8531]
["5.16","Very High",8532]
["5.17","Very High",8533]
["5.18","High",8534]
["5.19","Medium",8535]
["5.2","Very High",8518]
["5.20","Medium",8536]
["5.21","Medium",8537]
["5.22","High",8539]
["5.23","Very High",8540]
["5.24","Very High",8541]
["5.25","Medium",8542]
["5.26","Medium",8543]
["5.27","Medium",8544]
["5.28","Very High",8545]
["5.29","High",8546]
["5.3","Low",8519]
["5.30","High",8547]
["5.31","High",8548]
["5.32","High",8549]
["5.33","High",8550]
["5.34","Low",8551]
["5.35","Medium",8552]
["5.36","Low",8553]
["5.37","Low",8554]
["5.38","High",8555]
["5.39","Very High",8556]
["5.4","High",8520]
["5.40","Very High",8557]
["5.41","Very High",8558]
["5.42","Medium",8559]
["5.43","High",8560]
["5.44","High",8561]
["5.45","Medium",8564]
["5.46","Medium",8565]
["5.47","Medium",8566]
["5.48","Medium",8567]
["5.5","Low",8521]
["5.6","Low",8522]
["5.7","Medium",8523]
["5.8","Medium",8524]
["5.9","Very High",8525]
["5.99","High",8568]
["6.1","Medium",8348]
["6.10","Low",8357]
["6.11","High",8358]
["6.12","Medium",8359]
["6.13","Low",8360]
["6.14","High",8361]
["6.15","High",8362]
["6.16","Very High",8363]
["6.17","Very High",8364]
["6.18","Medium",8365]
["6.19","Low",8366]
["6.2","High",8349]
["6.20","Medium",8367]
["6.21","High",8368]
["6.22","Medium",8369]
["6.3","Low",8350]
["6.4","High",8351]
["6.5","Medium",8352]
["6.6","Medium",8353]
["6.7","High",8354]
["6.8","High",8355]
["6.9","Low",8356]
["6.99","High",8370]
["7.1","High",8371]
["7.10","High",8380]
["7.11","High",8381]
["7.12","High",8382]
["7.13","Medium",8383]
["7.14","Medium",8384]
["7.15","High",8385]
["7.16","High",8386]
["7.17","High",8387]
["7.2","High",8372]
["7.3","Low",8373]
["7.4","Low",8374]
["7.5","Low",8375]
["7.6","Medium",8376]
["7.7","Low",8377]
["7.8","High",8378]
["7.9","High",8379]
["7.99","High",8388]
["8.1","Very High",8569]
["8.10","Very High",8578]
["8.100","Low",11227]
["8.101","Medium",11228]
["8.102","Low",11229]
["8.103","Low",11230]
["8.104","Low",11231]
["8.105","Medium",11232]
["8.106","Medium",11233]
["8.107","Low",11234]
["8.108","High",11235]
["8.109","Very High",11236]
["8.11","Medium",8579]
["8.110","High",11237]
["8.111","Medium",11238]
["8.112","High",11239]
["8.113","Medium",11240]
["8.114","Low",11241]
["8.115","High",11242]
["8.116","Medium",11243]
["8.117","Medium",11244]
["8.118","Medium",11245]
["8.119","High",11246]
["8.12","Medium",8580]
["8.120","High",11247]
["8.121","Medium",11248]
["8.122","High",11249]
["8.123","High",11250]
["8.124","Low",11251]
["8.125","High",11252]
["8.126","Medium",11253]
["8.127","Medium",11254]
["8.13","Medium",8581]
["8.14","Very High",8582]
["8.15","High",8583]
["8.16","Very High",8584]
["8.17","Low",8585]
["8.18","High",8586]
["8.19","High",8587]
["8.199","High",11255]
["8.2","Medium",8570]
["8.20","Medium",8588]
["8.21","High",8589]
["8.22","Very High",8590]
["8.23","Medium",8591]
["8.24","Medium",8592]
["8.25","Very High",8593]
["8.26","High",8594]
["8.27","Medium",8595]
["8.28","Medium",8596]
["8.29","High",8598]
["8.3","Very High",8571]
["8.30","High",8599]
["8.31","High",8600]
["8.32","Low",8601]
["8.33","Medium",8602]
["8.34","High",8603]
["8.35","Medium",8604]
["8.36","Medium",8605]
["8.37","High",8607]
["8.38","Medium",8608]
["8.39","Medium",8609]
["8.4","Medium",8572]
["8.40","High",8610]
["8.41","Medium",8611]
["8.42","Medium",8612]
["8.43","Very High",8613]
["8.44","High",8615]
["8.45","High",8616]
["8.46","Very High",8617]
["8.47","Very High",8618]
["8.48","Medium",8619]
["8.49","High",8620]
["8.5","Very High",8573]
["8.50","Medium",8621]
["8.51","Low",8622]
["8.52","Low",8623]
["8.53","Low",8624]
["8.54","High",8625]
["8.55","Low",11182]
["8.56","Medium",11183]
["8.57","Medium",11184]
["8.58","High",11185]
["8.59","High",11186]
["8.6","Medium",8574]
["8.60","High",11187]
["8.61","Medium",11188]
["8.62","Very High",11189]
["8.63","High",11190]
["8.64","Medium",11191]
["8.65","Low",11192]
["8.66","High",11193]
["8.67","High",11194]
["8.68","High",11195]
["8.69","Medium",11196]
["8.7","High",8575]
["8.70","Medium",11197]
["8.71","Very High",11198]
["8.72","Medium",11199]
["8.73","Medium",11200]
["8.74","High",11201]
["8.75","Medium",11202]
["8.76","Medium",11203]
["8.77","Medium",11204]
["8.78","Medium",11205]
["8.79","Medium",11206]
["8.8","Medium",8576]
["8.80","Medium",11207]
["8.81","Low",11208]
["8.82","Medium",11209]
["8.83","Low",11210]
["8.84","Low",11211]
["8.85","Medium",11212]
["8.86","Medium",11213]
["8.87","Medium",11214]
["8.88","Low",11215]
["8.89","High",11216]
["8.9","High",8577]
["8.90","High",11217]
["8.91","High",11218]
["8.92","Medium",11219]
["8.93","Low",11220]
["8.94","Low",11221]
["8.95","Medium",11222]
["8.96","Medium",11223]
["8.97","Low",11224]
["8.98","High",11225]
["8.99","Medium",11226]
["9.1","Low",8390]
["9.10","Medium",8399]
["9.11","Medium",8400]
["9.12","Medium",8401]
["9.13","Low",8402]
["9.14","Medium",8403]
["9.15","Medium",8404]
["9.16","High",8405]
["9.17","High",8406]
["9.18","Low",8407]
["9.19","Low",8408]
["9.2","Very High",8391]
["9.20","Medium",8409]
["9.21","Medium",8410]
["9.22","Low",8411]
["9.23","Low",8412]
["9.24","Medium",8413]
["9.25","Low",8414]
["9.26","Low",8415]
["9.27","Low",8416]
["9.28","Medium",8417]
["9.29","Low",8418]
["9.3","Very High",8392]
["9.4","High",8393]
["9.5","High",8394]
["9.6","Low",8395]
["9.7","Medium",8396]
["9.8","Medium",8397]
["9.9","Medium",8398]
["9.99","High",8419]

{"sheet":"Equipment_list","index":7,"n_rows":28,"n_cols":3,"rows_kept":28,"cut":false,"hidden":true,"merged":[]}
["TITLE","Equipment_list_description","ID"]
["Accommodation",null,12]
["Cargo Mach.",null,13]
["Critical Equip.",null,16]
["Deck - Machinery",null,18]
["Deck - Mooring Machinery",null,15]
["Deck - Pipe / Fittings",null,20]
["Documentation",null,21]
["E/R - Air Comp.",null,8]
["E/R - Aux. Engine",null,4]
["E/R - Aux. Mach.",null,7]
["E/R - Boiler",null,5]
["E/R - Main Engine",null,3]
["E/R - Pipes/ valves & fittings",null,9]
["E/R - Pumps",null,32]
["E/R - Purifier",null,6]
["Elect. Mach. & Equip.",null,10]
["Hull & Tanks",null,19]
["Inert Gas",null,14]
["LSA / FFA",null,17]
["Miscellaneous",null,22]
["Navigation - DGPS / EPFS / AIS",null,28]
["Navigation - ECDIS",null,25]
["Navigation - Echo Sounder / Speed Log",null,26]
["Navigation - GMDSS & Communication",null,23]
["Navigation - Others",null,11]
["Navigation - RADAR",null,24]
["Navigation - VDR / BNWAS",null,30]

{"sheet":"PSC_MOU","index":8,"n_rows":11,"n_cols":3,"rows_kept":11,"cut":false,"hidden":true,"merged":[]}
["TITLE","PSC_MOU_description","ID"]
["Asia and the Pacific",null,2]
["Caribbean",null,4]
["Europe and the North Atlantic",null,1]
["Latin America",null,3]
["The Black Sea region",null,6]
["The Indian Ocean",null,8]
["The Mediterranean",null,7]
["The Riyadh MoU",null,9]
["USCG",null,10]
["West and Central Africa",null,5]

{"sheet":"Inspection_type","index":9,"n_rows":13,"n_cols":2,"rows_kept":13,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Bunkering Audit",14]
["Cargo Audit",17]
["Engineering Audit",16]
["ISM Audit",2]
["ISPS Audit",3]
["IT Audit",10]
["MLC Audit",1]
["Mooring Audit",9]
["Nav Audit / Verification",8]
["Onboard Training",18]
["Ship Staff Insp.",15]
["Suptd. Insp.",13]

{"sheet":"Deficiency_Cause","index":10,"n_rows":8,"n_cols":3,"rows_kept":8,"cut":false,"hidden":true,"merged":[]}
["TITLE","Deficiency_Cause_description","ID"]
["Behaviour Based",null,1]
["Equipment Related",null,4]
["External Factors",null,5]
["Human Error",null,7]
["Inappropriate Procedure",null,8]
["Industry Issue",null,6]
["Knowledge Based",null,3]

{"sheet":"Observer_code","index":11,"n_rows":3,"n_cols":3,"rows_kept":3,"cut":false,"hidden":true,"merged":[]}
["TITLE","Observer_code_description","ID"]
["Owner / Marine / Tech. Suptd.",null,3]
["Ship Staff",null,2]

{"sheet":"Status_code","index":12,"n_rows":6,"n_cols":3,"rows_kept":6,"cut":false,"hidden":true,"merged":[]}
["TITLE","Status_code_description","ID"]
["Completed",null,6]
["Deferred to D D",null,5]
["In progress",null,3]
["Not Started",null,2]
["Waiting spare",null,4]

{"sheet":"PSC_ref_no","index":13,"n_rows":19,"n_cols":2,"rows_kept":19,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Alarms",9]
["Cargo operations including equipment",7]
["Certificates & Documentation",2]
["Dangerous Goods",13]
["Emergency Systems",5]
["Fire safety",8]
["ISM",16]
["ISPS",17]
["Life saving appliances",12]
["MLC, 2006",18]
["Other",19]
["Pollution Prevention",15]
["Propulsion and auxiliary machinery",14]
["Radio communication",6]
["Safety of Navigation",11]
["Structural condition",3]
["Water/Weathertight condition",4]
["Working and Living Conditions",10]

{"sheet":"Risk_value_of_obs","index":14,"n_rows":1,"n_cols":2,"rows_kept":1,"cut":false,"hidden":true,"merged":[]}
["Risk Value of observation","ID"]

{"sheet":"Year","index":15,"n_rows":18,"n_cols":1,"rows_kept":18,"cut":false,"hidden":true,"merged":[]}
["Year"]
[2014]
[2015]
[2016]
[2017]
[2018]
[2019]
[2020]
[2021]
[2022]
[2023]
[2024]
[2025]
[2026]
[2027]
[2028]
[2029]
[2030]

{"sheet":"Month","index":16,"n_rows":13,"n_cols":1,"rows_kept":13,"cut":false,"hidden":true,"merged":[]}
["Month"]
["Jan"]
["Feb"]
["Mar"]
["Apr"]
["May"]
["Jun"]
["Jul"]
["Aug"]
["Sep"]
["Oct"]
["Nov"]
["Dec"]

{"sheet":"Date_","index":17,"n_rows":32,"n_cols":1,"rows_kept":32,"cut":false,"hidden":true,"merged":[]}
["Date"]
["01"]
["02"]
["03"]
["04"]
["05"]
["06"]
["07"]
["08"]
["09"]
[10]
[11]
[12]
[13]
[14]
[15]
[16]
[17]
[18]
[19]
[20]
[21]
[22]
[23]
[24]
[25]
[26]
[27]
[28]
[29]
[30]
[31]

{"sheet":"Sheet1","index":18,"n_rows":24,"n_cols":6,"rows_kept":24,"cut":false,"hidden":true,"merged":[]}
[]
[null,"ID","E",null,"Date Recorded",1]
[null,"UNIQUE ID","F",null,"Type of Deficiency",2]
[1,"Date Recorded","G",null,"Observer code",3]
["ignore","Vessel Type","H",null,"Type of Inspection",4]
[null,"Internal / External","I",null,"Description of Deficiency",5]
[null,"Drydock","J",null,"Equipment Categories",6]
[null,"Information Sharing","K",null,"Area of Observation",7]
[null,"Critical_item","L",null,"Deficiency Cause",8]
[null,"Deficiency Type","M",null,"VIQ Ref Number",9]
[null,"Deficiency Cause","N",null,"Risk Value of Obs",10]
[null,"Inspection Type","O",null,"PSC Ref Number",11]
[null,"Equipments","P",null,"PSC MOU ID",12]
[null,"VIQ Reference Number","Q",null,"Action Taken or Required",13]
[null,"Risk Value of the observation","R",null,"Target Date",14]
[null,"PSC Reference Number","S",null,"PO Ref No.",15]
[null,"PSC MOU","T",null,"Status Code",16]
[null,"Observer Code","U",null,"Date Completed",17]
[null,"Target Date","V",null,"Drydock",18]
[null,"Status Code","W",null,"Info Sharing",19]
[null,"Description of Deficiency","X",null,"Critical Item Flag",20]
[null,"Action taken / required","Y",null,"Audit Type",21]
[null,"PO ref no","Z"]
[null,"Date completed","AA"]

{"sheet":"Ship_information","index":19,"n_rows":2,"n_cols":3,"rows_kept":2,"cut":false,"hidden":true,"merged":[]}
["Ship_ID","Ship_Name","FILE_NAME"]
["45","DHT SCANDINAVIA (22-04-2022)","45_1650873801153.xlsm"]

{"sheet":"External_Deficiency_type","index":20,"n_rows":5,"n_cols":3,"rows_kept":5,"cut":false,"hidden":true,"merged":[]}
["TITLE","Type of deficiency_description","ID"]
["Condn of Class / Memo",null,5]
["Defect",null,1]
["Non Conformity",null,2]
["Observation",null,3]

{"sheet":"External_Inspection_type","index":21,"n_rows":11,"n_cols":2,"rows_kept":11,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Cargo Audit",17]
["Flag State Insp.",5]
["ISM Audit",2]
["ISPS Audit",3]
["MLC Audit",1]
["Nav Audit / Verification",8]
["OM Insp. (Eg. SIRE / CDI etc.)",6]
["Others (Eg. Insurance etc.)",12]
["PSC Inspection",4]
["Terminal Insp.",11]

{"sheet":"External_Observer_code","index":22,"n_rows":7,"n_cols":3,"rows_kept":7,"cut":false,"hidden":true,"merged":[]}
["TITLE","Observer_code_description","ID"]
["Class Surveyor",null,4]
["FSC Inspector",null,5]
["Others (Eg. Insurance etc.)",null,9]
["PSC Insp.",null,6]
["SIRE / CDI Insp.",null,8]
["Terminal Insp.",null,7]

{"sheet":"Sheet Version","index":23,"n_rows":2,"n_cols":2,"rows_kept":2,"cut":false,"hidden":true,"merged":[]}
["Version","Title"]
["2.0","Version 2.0"]