{"text_format":"1","workbook":"xlsx","n_sheets":24,"sheets":["Mainsheet","Completed","Calc","Areaofobs","Vessel_type","Deficiency_type","VIQrefno","Equipment_list","PSC_MOU","Inspection_type","Deficiency_Cause","Observer_code","Status_code","PSC_ref_no","Risk_value_of_obs","Year","Month","Date_","Sheet1","Ship_information","External_Deficiency_type","External_Inspection_type","External_Observer_code","Sheet Version"],"not_rendered":{"charts":0,"images":1,"macros":1,"external_links":0,"defined_names":12,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Mainsheet","index":0,"n_rows":36,"n_cols":28,"rows_kept":36,"cut":false,"hidden":false,"merged":[[10,8,10,9],[10,12,10,13],[12,6,12,27],[8,6,8,27]]}
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,"Defect - Damage Monitoring Sheet"]
[]
[null,null,null,null,null,null,null,"Date of Report","02-Mar-2023",null,null,"Ship Name","MOJO (19-05-2022)"]
[]
[null,null,null,null,null,null,"VERSION : 2.0"]
[]
[]
[]
[null,null,null,"ID","SHIPSIDE UNIQUEID","UNIQUE ID","Date Recorded","Type of Deficiency","Observer code","Type of Inspection","Description of Deficiency","Equipment Categories","Area of Observation","Deficiency Cause","VIQ Ref Number","Risk Value of Obs","PSC Ref Number","PSC MOU ID","Action Taken or Required","Target Date","PO Ref No.","Status Code","Date Completed","Drydock","Info Sharing","Critical Item","Audit Type","Superintendent Remarks"]
[null,null,null,null,76455,"0_Wed Jan 11 2023 11:39:04 GMT+0800","2023-01-01T08:00:00","Defect","Ship Staff","Ship Staff Insp.","CARGO HOLD HATCH COVERS CHAINS TO BE RENEWED","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","CHAINS RECEIVED TO BE CHANGED","2023-02-28T08:00:00","","In progress",null,"No","No","No","Internal"]
[null,null,null,null,22100,"0_Wed Jan 11 2023 11:43:15 GMT+0800","2023-01-01T08:00:00","Defect","Ship Staff","Ship Staff Insp.","WATER MIST PANEL ON BRIDGE DIMMER SWITCH NOT WORKING","LSA / FFA","Emgcy. Systems","Equipment Related","","","","","SPARE PART ORDERED BUT RECEIVED WRONG SUPPLY . RO no. MOJO220181  ","2023-02-28T08:00:00","","Waiting spare",null,"No","No","No","Internal"]
[null,null,null,null,79801,"93_Wed Jan 11 2023 14:00:45 GMT+0800","2023-01-01T08:00:00","Critical Equipment","Ship Staff","Ship Staff Insp.","P.A SYSTEM SPEAKER BASE BROKEN WHICH NEEDS TO BE REPLACED.","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","REQ RAISED FOR THE SPARE PARTS. VESSEL AWAITING PARTS TO BE DELIVERED. RO No. MOJO230002","2023-02-28T08:00:00","","Waiting spare",null,"No","No","No","Internal"]
[null,null,null,null,96602,"93_Wed Jan 11 2023 16:11:48 GMT+0800","2023-01-10T08:00:00","Critical Equipment","Ship Staff","Ship Staff Insp.","water ingress alarm system faulty","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","WIA system attended by service engineer at Dry dock. All faults in the system rectified and system working satisfactorily","2023-02-22T08:00:00","","In progress","2023-01-20T08:00:00","No","No","No","Internal"]
[null,null,null,null,84726,"93_Wed Jan 11 2023 17:36:57 GMT+0800","2022-12-23T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Galley baking oven low insulation","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","upon inspection, found that the low insulation is from the heater. RO has been raised for the same. RO no. MOJO220293","2023-01-31T08:00:00","","In progress",null,"No","No","No","Internal"]
[null,null,null,null,60004,"93_Fri Jan 27 2023 11:38:39 GMT+0800","2023-01-27T08:00:00","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","No.6 cargo hatch cover under side to be de-rusted and\npainted.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","Will be de rusted and painted once vessel is in calm sea and hatch covers can be opened.","2023-03-27T08:00:00","","Not Started",null,"No","No","No","Internal"]
[null,null,null,null,23090,"0_Fri Jan 27 2023 11:49:54 GMT+0800","2023-01-26T08:00:00","Observation","Ship Staff","Suptd. Insp.","Provision crane hoisting limit switch to be greased","Deck - Machinery","General Appearance","Equipment Related","","","","","Provision crane limit switches to be greased regularly ","2023-03-28T08:00:00","","Not Started",null,"No","No","No","Internal"]
[null,null,null,null,28538,"0_Fri Jan 27 2023 11:58:44 GMT+0800","2023-01-26T08:00:00","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","All hatch cover jack up cylinder mounting foundation to be\nde-rusted and coated.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","All hatch cover jack up cylinder mounting foundation to be\nDe-rusted and painted at calm sea / anchorage","2023-03-23T08:00:00","","In progress",null,"No","No","No","Internal"]
[null,null,null,null,16782,"0_Fri Jan 27 2023 12:07:47 GMT+0800","2023-01-27T08:00:00","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","All mooring winch directional control block to be de-rusted\nand coated.","Deck - Mooring Machinery","Mooring","Equipment Related","","","","","All mooring winch directional control block to be de-rusted\nand coated. to be carried out after hold cleaning","2023-02-28T08:00:00","","In progress",null,"No","No","No","Internal"]
[null,null,null,null,80387,"93_Fri Jan 27 2023 16:53:16 GMT+0800","2023-01-27T08:00:00","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Engine room bilge well to be cleaned thoroughly, make sure free of oil.","E/R - Pipes/ valves & fittings","MARPOL Related","Inappropriate Procedure","","","","","Bilge well to be transferred to OBT and bilge well to be cleaned thoroughly.","2023-02-03T08:00:00","","In progress",null,"No","No","No","Internal"]
[null,null,null,null,38819,"93_Fri Jan 27 2023 18:13:03 GMT+0800","2023-01-27T08:00:00","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Newly installed BWTS pipe to be painted.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","BWTS pipelines to be painted.","2023-02-26T08:00:00","","Not Started",null,"No","No","No","Internal"]
[null,null,null,null,36817,"93_Fri Jan 27 2023 18:17:19 GMT+0800","2023-01-27T08:00:00","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","PMS to be updated for machinery maintenance record after docking repair.","Documentation","ISM Related","Equipment Related","","","","","Machinery maintenance record to be updated in PMS.","2023-02-11T08:00:00","","Not Started",null,"No","No","No","Internal"]
[null,null,null,null,91504,"93_Fri Jan 27 2023 18:20:32 GMT+0800","2023-01-27T08:00:00","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Spare parts status to be updated in PAL after docking repair.","Documentation","ISM Related","Equipment Related","","","","","Spares received and consumed during maintenance at dry dock  to be updated in PAL.","2023-02-11T08:00:00","","Not Started",null,"No","No","No","Internal"]
[null,null,null,null,19490,"0_Fri Feb 17 2023 16:49:04 GMT+0800","2023-02-16T08:00:00","Non Conformity","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Maindeck, hatch cover number four,helicopter landing area\nmarking was not complied with ICS guidelines.","Miscellaneous","ISM Related","Inappropriate Procedure","","","","","Same was reported to company to confirm with class, if vessel can change the marking for helicopter landing area. once conformation received the marking will be changed as required. ","2023-04-30T08:00:00","","In progress",null,"No","No","No","Internal"]
[null,null,null,null,89558,"0_Fri Feb 17 2023 16:53:36 GMT+0800","2023-02-16T08:00:00","Non Conformity","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Maindeck, hatch cover hydraulic equipment was not\nprovided with adequate containment arrangements around\nthe base.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","HYD JACKS FOR HATCH COVER WERE NOT PROVIDED WITH DRIP TRAY ARRANGEMENT. SAME IS TO BE CONFIRMED WITH COMPANY IF VESSEL CAN MAKE THE ARRANGEMENT FOR THE SAME OR TO BE DONE AT NEXT DRY DOCK.","2023-04-30T08:00:00","","In progress",null,"No","No","No","Internal"]
[null,null,null,null,26883,"0_Fri Feb 17 2023 16:54:57 GMT+0800","2023-02-16T08:00:00","Non Conformity","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Mooring line LDBF on board was observed 114% of the\nship's designed maximum breaking limit.","Deck - Mooring Machinery","Cert. & Docu.","Equipment Related","","","","","SAME IS INFORMED THE COMPANY VESSEL AWAITING RESPONSE.","2023-04-30T08:00:00","","In progress",null,"No","No","No","Internal"]
[null,null,null,null,25746,"93_Tue Feb 28 2023 11:43:43 GMT+0800","2023-02-10T08:00:00","Defect","Ship Staff","Ship Staff Insp.","THE MAIN ENGINE FO FLOW METER NOT WORKING","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","NEED TO BE OVERHAULED/REPLACED","2023-04-20T08:00:00","","Not Started",null,"No","No","No","Internal"]
[null,null,null,null,68152,"93_Tue Feb 28 2023 11:45:36 GMT+0800","2023-02-10T08:00:00","Observation","Ship Staff","Ship Staff Insp.","THE BOILER FO FLOW METER NOT WORKING","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","NEED TO BE OVERHAULED/ REPLACED","2023-04-19T08:00:00","","Not Started",null,"No","No","No","Internal"]
[null,null,null,null,84232,"93_Tue Feb 28 2023 11:53:12 GMT+0800","2023-02-13T08:00:00","Observation","Ship Staff","Ship Staff Insp.","BOILER FO LOW PR IN BURNER PR SWITCH DAMAGED","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","SAME NEED TO BE REPLACED","2023-04-26T08:00:00","MOJO230046","Waiting spare",null,"No","No","No","Internal"]

{"sheet":"Completed","index":1,"n_rows":562,"n_cols":28,"rows_kept":562,"cut":false,"hidden":false,"merged":[[10,8,10,9],[10,12,10,13],[12,6,12,27],[8,6,8,27]]}
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,"Defect - Damage Monitoring Sheet"]
[]
[null,null,null,null,null,null,null,"Date of Report","02-Mar-2023",null,null,"Ship Name","MOJO (19-05-2022)"]
[]
[null,null,null,null,null,null,"VERSION : 2.0"]
[]
[]
[]
[null,null,null,"ID","SHIPSIDE UNIQUEID","UNIQUE ID","Date Recorded","Type of Deficiency","Observer code","Type of Inspection","Description of Deficiency","Equipment Categories","Area of Observation","Deficiency Cause","VIQ Ref Number","Risk Value of Obs","PSC Ref Number","PSC MOU ID","Action Taken or Required","Target Date","PO Ref No.","Status Code","Date Completed","Drydock","Info Sharing","Critical Item","Audit Type","Superintendent Remarks"]
[null,null,null,7555,null,"93_Tue Feb 12 2019 09:40:32 GMT+0000 (Coordinated Universal Time)","2019-01-15T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Hull stress monitor is already decommissioned, all fittings on deck & bridge to be removed at DD","Deck - Pipe / Fittings","General Appearance","Equipment Related","","","","","HSMS fittings cropped from the deck and removed by Ship tard.","2020-03-31T23:59:35","","Completed","2020-04-07T23:59:35","Yes","No","No","Internal"]
[null,null,null,7542,null,"93_Mon Dec 02 2019 19:23:23 GMT+0000 (Coordinated Universal Time)","2019-08-14T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Hull Paint in Poor Condition, especially topsides all around. ","Hull & Tanks","Structural Condn. / WT integrity ","External Factors","","","","","Hull painted in Dry dock after high pressure wash and sand blasting.","2020-01-31T23:59:35","","Completed","2020-01-19T23:59:35","Yes","No","No","Internal"]
[null,null,null,7543,null,"93_Tue Feb 12 2019 19:27:34 GMT+0000 (Coordinated Universal Time)","2019-08-15T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Both ECDIS UPS, expiring in jan 2020","Navigation - ECDIS","Navigation","Equipment Related","","","","","ECDIS UPS changed by ETO. ","2020-03-31T23:59:35","007D/19","Completed","2020-03-10T23:59:35","No","No","No","Internal"]
[null,null,null,7544,null,"93_Tue Feb 12 2019 21:08:57 GMT+0000 (Coordinated Universal Time)","2019-08-15T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Elevator to be recommissioned as per flag state requirements.","Miscellaneous","General Appearance","Equipment Related","","","","","Invetor and the PCB renewed by the shore technician, elevator made operational.","2020-03-31T23:59:35","","Completed","2020-03-31T23:59:35","Yes","No","No","Internal"]
[null,null,null,7545,null,"93_Tue Feb 12 2019 08:49:02 GMT+0000 (Coordinated Universal Time)","2019-08-15T23:59:35","Defect","Ship Staff","Ship Staff Insp.","All Cargo holds show heavy rusting, including but not limited to CH booby hatch access, rubber packing retaining channel, Australian ladders / straight ladders & guard pipes show heavy corrosion & total wasting at many places. ","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","All cargo holds, Cleaned with high pressure fresh water wash and grit blasted. The cargo holds, along with the Australian and Vertical ladders, Pipes and supports, Upperstool areas were painted with 2 coats of cargo hold paint as per specification.","2020-03-31T23:59:35","","Completed","2020-04-01T23:59:35","Yes","No","No","Internal"]
[null,null,null,7546,null,"93_Tue Feb 12 2019 08:51:39 GMT+0000 (Coordinated Universal Time)","2019-08-15T23:59:35","Defect","Ship Staff","Ship Staff Insp.","All hatch cover packings & CH access hatch packings are hardened & grooved (Loss of resilience) & also  understand have few leakages. Also packing retaining channel totally wasted at many places. ","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","All hatch cover & hatch access lid packings  renewed & packing retaining channel full derusted, cropped & renewed & painted as required.","2020-03-31T23:59:35","","Completed","2020-04-13T23:59:35","Yes","No","No","Internal"]
[null,null,null,7547,null,"93_Tue Feb 12 2019 08:53:08 GMT+0000 (Coordinated Universal Time)","2019-08-15T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Both windlass brake bands worn out by 70%. ","Deck - Mooring Machinery","Mooring","Equipment Related","","","","","Both windlass brake bands renewed in DD. ","2020-03-31T23:59:35","","Completed","2020-04-13T23:59:35","Yes","No","No","Internal"]
[null,null,null,7548,null,"93_Tue Feb 12 2019 08:56:34 GMT+0000 (Coordinated Universal Time)","2019-08-15T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Bridge sofa, Crew Mess Room, completely torn & upholstery held in place with tapes. Bridge radio station chair, ship's office chair, ECR chair to be replaced. ","Miscellaneous","General Appearance","Equipment Related","","","","","All sofas and chairs mentioned re-upholstered and attended in DD.","2020-03-31T23:59:35","","Completed","2020-04-08T23:59:35","Yes","No","No","Internal"]
[null,null,null,7549,null,"93_Tue Feb 12 2019 09:30:42 GMT+0000 (Coordinated Universal Time)","2019-08-15T23:59:35","Defect","Ship Staff","Ship Staff Insp.","On stbd side stern frame, steering gear room bulkhead shows an indentation & slight bending of longitudinal (area about 02m x 02m)","Hull & Tanks","Structural Condn. / WT integrity ","Equipment Related","","","","","Class surveyor and Owners are satisfied with the condition. Hence the job has been cancelled.","2020-01-31T23:59:35","","Completed","2020-01-10T23:59:35","Yes","No","No","Internal"]
[null,null,null,7550,null,"93_Tue Feb 12 2019 09:32:41 GMT+0000 (Coordinated Universal Time)","2019-08-15T23:59:35","Defect","Ship Staff","Ship Staff Insp.","There is no solid fairlead on forecastle deck P&S side to pass tug boat towing lines. Similarly no solid centre lead on poop deck. It was observed vessel passes tug towing lines on forecastle deck & poop deck via roller fairleads, which are not designed for tug pulling stress. ","Deck - Mooring Machinery","Mooring","Equipment Related","","","","","Owners are satisfied with the mooring arrangement onboard. hence no modifications are required. job cancelled.","2020-01-31T23:59:35","","Completed","2020-01-10T23:59:35","Yes","No","No","Internal"]
[null,null,null,7551,null,"93_Mon Dec 02 2019 09:34:21 GMT+0000 (Coordinated Universal Time)","2019-08-15T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Aft P side stern rope winch on poop dk & spring rope mooring winch between hatch no.08 & 09 - Control lever unit trickle leaking oil, also for aft breast line, stern lines, spring mooring winch gear engaging clutch lever base welding to main body has come off. ","Deck - Mooring Machinery","Mooring","Equipment Related","","","","","Control lever checked for leaking seal & all control blocks overhauled and serviced by attending technicians in DD.","2020-03-31T23:59:35","","Completed","2020-04-13T23:59:35","No","No","No","Internal"]
[null,null,null,7552,null,"93_Tue Feb 12 2019 09:35:52 GMT+0000 (Coordinated Universal Time)","2019-08-15T23:59:35","Defect","Ship Staff","Ship Staff Insp.","All mooring winches hydraulic motor gearbox oil seems to be curdled, no record of renewal.","Deck - Mooring Machinery","Mooring","Equipment Related","","","",""," 6 winches oil renewed. ","2020-08-31T23:59:35","","Completed","2020-06-09T23:59:35","Yes","No","No","Internal","Job completed by shipstaff during docking, update job accordingly."]
[null,null,null,7553,null,"93_Tue Feb 12 2019 09:37:17 GMT+0000 (Coordinated Universal Time)","2019-08-15T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Mooring winches hydraulic motor gearbox oil filling cap  frozen stiff in place & suspect to be wasted. ","Deck - Mooring Machinery","Mooring","Equipment Related","","","","","All filling caps in good condition and oil renewed in windlass and gangway gear box.","2020-03-31T23:59:35","","Completed","2020-04-13T23:59:35","Yes","No","No","Internal"]
[null,null,null,7554,null,"93_Tue Feb 12 2019 09:38:52 GMT+0000 (Coordinated Universal Time)","2019-08-15T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Spare anchor to be off landed in DD.","Deck - Mooring Machinery","Mooring","Equipment Related","","","","","Spare anchor is in good condition. De-rusted and painted by Yard. Owners did not approve for landing the spare anchor. Hence the job is cancelled.","2020-01-31T23:59:35","","Completed","2020-01-10T23:59:35","Yes","No","No","Internal"]
[null,null,null,7672,null,"93_Mon Dec 02 2019 21:02:39 GMT+0000 (Coordinated Universal Time)","2019-08-15T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Gyro Compass Annual servicing over due since July 2019","Navigation - Others","Navigation","Equipment Related","","","","","Gyro Compass servicing & gyrosphere replaced with reconditioned gyrosphere at Xiamen.","2019-09-15T23:59:35","002D/19","Completed","2019-11-13T23:59:35","No","No","No","Internal"]
[null,null,null,7556,null,"93_Tue Feb 12 2019 09:42:18 GMT+0000 (Coordinated Universal Time)","2019-08-19T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Almost all hatch cover not sitting on resting pads. Hatch cover lip resting on hatch coaming at many places","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","Resting pads rebuilt as required & all hatch cover packings renewed. Chalk test carried out and found satisfactory.","2020-03-31T23:59:35","","Completed","2020-04-13T23:59:35","Yes","No","No","Internal"]
[null,null,null,7558,null,"93_Tue Feb 12 2019 09:46:37 GMT+0000 (Coordinated Universal Time)","2019-08-19T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Many hatch cover hydraulic lifting jack leaking from seal. ","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","All flexible hoses & seals of hatch cover lifting jacks renewed. Lifting jacks removed from location for servicing and rechroming  by ship yard. All seals renewed. ","2020-03-31T23:59:35","","Completed","2020-04-13T23:59:35","Yes","No","No","Internal"]
[null,null,null,7559,null,"93_Tue Feb 12 2019 09:49:56 GMT+0000 (Coordinated Universal Time)","2019-08-19T23:59:35","Defect","Ship Staff","Ship Staff Insp.","All cargo holds hatch cover natural vents flame arrestors badly painted over","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","Wire mesh renewed once the new louvers were fitted back by the yard. ","2020-03-31T23:59:35","","Completed","2020-04-08T23:59:35","Yes","No","No","Internal"]
[null,null,null,7560,null,"93_Tue Feb 12 2019 09:51:46 GMT+0000 (Coordinated Universal Time)","2019-08-19T23:59:35","Defect","Ship Staff","Ship Staff Insp.","X band RADARS Magnetron due for renewal. (Last renewal in Nov 2017). S Band Radar PM not working","Navigation - RADAR","Navigation","Equipment Related","","","","","X band magnetron renewed on 19-Jan-2020 and S Band PM renewed and replaced with new one and now working satisfactory.","2020-03-31T23:59:35","","Completed","2020-03-13T23:59:35","Yes","No","No","Internal"]
[null,null,null,7561,null,"93_Mon Dec 02 2019 09:53:55 GMT+0000 (Coordinated Universal Time)","2019-08-19T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Hatch cover drawing chains of following hatch covers full wasted & narrowed down (# 01PA, 02P&SF, 03, 04F, 05F, 07","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","",""," All wasted hatch cover drawing chains replaced with new ones as required. ","2020-03-31T23:59:35","","Completed","2020-05-15T23:59:35","Yes","No","No","Internal"]
[null,null,null,7562,null,"93_Tue Feb 12 2019 09:55:56 GMT+0000 (Coordinated Universal Time)","2019-08-19T23:59:35","Defect","Ship Staff","Ship Staff Insp.","No.04 & 02 hatch covers drawing hydraulic motor is leaking oil continuously from flexible pipe joint. ","Deck - Mooring Machinery","Cargo / Ballast Systems","Equipment Related","","","","","All hatch cover hydraulic drawing chain motor bushes, bearings & seal renewed as required.","2020-03-31T23:59:35","017E/19","Completed","2020-04-13T23:59:35","No","No","No","Internal"]
[null,null,null,7563,null,"93_Tue Feb 12 2019 09:58:13 GMT+0000 (Coordinated Universal Time)","2019-08-19T23:59:35","Defect","Ship Staff","Ship Staff Insp.","04 nos. Drinking water fountains in accommodation to be made operational. ","Accommodation","MLC Related","Equipment Related","","","","","Drinking water fountain has no filter and candle for purifying. It is a simple water cooler. Water coolers working satisfactorily.","2020-03-31T23:59:35","","Completed","2020-04-13T23:59:35","Yes","No","No","Internal"]
[null,null,null,7564,null,"93_Mon Dec 02 2019 10:02:33 GMT+0000 (Coordinated Universal Time)","2019-08-19T23:59:35","Defect","Ship Staff","Ship Staff Insp.","All cabins porthole curtains found dirty & velcro tape has lost resilience, unable to completely block out light. ","Miscellaneous","MLC Related","Equipment Related","","","","","All curtains to be washed & cleaned. Velcro issue not needed.Navigation at night is not impeded. ","2020-08-31T23:59:35","","Completed","2020-04-13T23:59:35","No","No","No","Internal"]
[null,null,null,7565,null,"93_Mon Dec 02 2019 10:12:12 GMT+0000 (Coordinated Universal Time)","2019-08-19T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Many cabins clocks not synchronizing with bridge slave clock & requires manual adjustment. For eg: Owner's cabin. ","Miscellaneous","MLC Related","Equipment Related","","","","","Owners cancelled the job.","2020-03-31T23:59:35","","Completed","2020-04-13T23:59:35","Yes","No","No","Internal"]
[null,null,null,7566,null,"93_Tue Feb 12 2019 10:14:00 GMT+0000 (Coordinated Universal Time)","2019-08-19T23:59:35","Defect","Ship Staff","Ship Staff Insp.","No additional locking arrangement on the inside of accommodation alleyways exit doors abv A deck, for piracy prone areas. Same to be attended in DD as per company discretion.","Miscellaneous","ISPS Related","Equipment Related","","","","","To be done according to the trading area of the vessel.","2020-08-31T23:59:35","","Completed","2020-04-13T23:59:35","Yes","No","No","Internal","Docking is over, update job accordingly."]
[null,null,null,7567,null,"93_Mon Dec 02 2019 10:16:35 GMT+0000 (Coordinated Universal Time)","2019-08-19T23:59:35","Defect","Ship Staff","Ship Staff Insp.","FWG Ejector pump casing and motor in place,shaft, impeller, mechanical seal and coupling missing.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","",""," The shaft , impeller, mechanical seal and the coupling assembled and fitted back in place.The Pump tried out , found working satisfactory.The discharge pressure and amps found normal.","2020-01-31T23:59:35","003E/19","Completed","2020-01-25T23:59:35","No","No","No","Internal"]
[null,null,null,7568,null,"93_Mon Dec 02 2019 10:18:06 GMT+0000 (Coordinated Universal Time)","2019-08-19T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Aft Hydraulic Power Unit Oil  cooler sea water leaking from end cover","Deck - Mooring Machinery","Mooring","Equipment Related","","","","","The section of the leaking pipe at the end cover renewed, leak rectified","2020-03-31T23:59:35","","Completed","2020-02-26T23:59:35","Yes","No","No","Internal"]
[null,null,null,7569,null,"93_Mon Dec 02 2019 10:20:04 GMT+0000 (Coordinated Universal Time)","2019-08-19T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Emergency air driven diesel oil pump leaking. ","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Pump overhauled, the oil seal and O rings renewed and boxed back.","2020-03-31T23:59:35","006E/19","Completed","2020-03-29T23:59:35","Yes","No","No","Internal"]
[null,null,null,7570,null,"93_Tue Feb 12 2019 10:22:13 GMT+0000 (Coordinated Universal Time)","2019-08-19T23:59:35","Defect","Ship Staff","Ship Staff Insp.","It was observed Boiler burner unit is being held by chain block, whilst at sea","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","The burner unit pulled out and inspection carried out, found satisfactory. The burner unit need not be held by chain block","2020-03-31T23:59:35","","Completed","2020-02-02T23:59:35","Yes","No","No","Internal"]
[null,null,null,7571,null,"93_Tue Feb 12 2019 10:25:27 GMT+0000 (Coordinated Universal Time)","2019-08-19T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Aux. Engine fuel oil auto filter not in use.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","FO Filter control panel new  PCB and Transformer mounted in place and new candles and control elements changed with new spare received and Autofilter put in use.","2020-08-15T23:59:35","004 E / 19,  New RO- MOJO205038","Completed","2020-08-06T23:59:35","No","No","No","Internal","Spares ready & will be supplied at next convenient port."]
[null,null,null,7572,null,"93_Tue Feb 12 2019 10:27:32 GMT+0000 (Coordinated Universal Time)","2019-08-19T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Main Engine fuel oil line pressure regulator not working","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","",""," Pressure regulator renewed with new spare, now working satisfactory.","2020-03-31T23:59:35","005E/19","Completed","2020-02-26T23:59:35","Yes","No","No","Internal"]
[null,null,null,7573,null,"93_Tue Feb 12 2019 10:29:31 GMT+0000 (Coordinated Universal Time)","2019-08-19T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Main Engine fuel oil viscometer fuel oil leaking from seal. ","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Fuel Oil Viscometer overhauled , shaft seal, O rings and bearings renewed. Now working satisfactory.","2020-03-31T23:59:35","007E/19","Completed","2020-04-20T23:59:35","No","No","No","Internal"]
[null,null,null,7574,null,"93_Mon Dec 02 2019 10:31:42 GMT+0000 (Coordinated Universal Time)","2019-08-19T23:59:35","Defect","Ship Staff","Ship Staff Insp.","DW Sterlizer not working.","E/R - Aux. Mach.","MLC Related","Equipment Related","","","","","  Germicidal lamp and the ballast renewed with new spare, found working satisfactory.","2020-03-31T23:59:35","MOJO 190002","Completed","2020-02-04T23:59:35","Yes","No","No","Internal"]
[null,null,null,7575,null,"93_Tue Feb 12 2019 10:33:17 GMT+0000 (Coordinated Universal Time)","2019-08-19T23:59:35","Defect","Ship Staff","Ship Staff Insp.","STBD side sea chest both CU & AL anodes need to be renewed. ","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","The CU and Al anodes of Stbd. sea chest renewed with new spare anodes.","2020-01-31T23:59:35","","Completed","2020-01-18T23:59:35","Yes","No","No","Internal"]
[null,null,null,7576,null,"93_Tue Feb 12 2019 10:35:22 GMT+0000 (Coordinated Universal Time)","2019-08-19T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Aft ICCP display showing module/system fault","Hull & Tanks","Structural Condn. / WT integrity ","Equipment Related","","","","","Aft ICCP Module renewed with new spare, now working satisfactory.","2020-03-31T23:59:35","","Completed","2020-02-22T23:59:35","Yes","No","No","Internal"]
[null,null,null,7577,null,"93_Mon Dec 02 2019 10:37:02 GMT+0000 (Coordinated Universal Time)","2019-08-19T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Control air dryer not working properly","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Control air dryer inspected, filters cleaned,found working satisfactory.","2020-03-31T23:59:35","013E/19","Completed","2020-03-05T23:59:35","Yes","No","No","Internal"]
[null,null,null,7671,null,"93_Tue Feb 12 2019 10:00:13 GMT+0000 (Coordinated Universal Time)","2019-08-19T23:59:35","Defect","Ship Staff","Ship Staff Insp.","AIS still showing fault in vessel speed feed.","Navigation - DGPS / EPFS / AIS","Navigation","Equipment Related","","","","","Newly received AIS installed by Shore technician at Xiamen.","2019-11-05T23:59:35","","Completed","2019-11-10T23:59:35","No","No","No","Internal"]
[null,null,null,8951,null,"93_Tue Feb 12 2019 10:31:42 GMT+0000 (Coordinated Universal Time)","2019-08-19T23:59:35","Defect","Ship Staff","Ship Staff Insp.","DW Sterlizer not working.","E/R - Aux. Mach.","MLC Related","Equipment Related","","","","","The germicidal lamp of the sterilizer renewed with new spare , working satisfactory.","2020-03-31T23:59:35","","Completed","2020-03-07T23:59:35","Yes","No","No","Internal"]
[null,null,null,7578,null,"93_Tue Feb 12 2019 10:41:05 GMT+0000 (Coordinated Universal Time)","2019-08-20T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Hatch cover opening / closing control lever boxes many corroded & wasted. For eg: No.02 & 05","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","",""," New boxes fabricated & corroded ones cropped & renewed by yard in DD","2020-03-31T23:59:35","","Completed","2020-04-11T23:59:35","Yes","No","No","Internal"]
[null,null,null,7579,null,"93_Tue Feb 12 2019 10:43:06 GMT+0000 (Coordinated Universal Time)","2019-08-20T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Air btl safety valve for QCV in fire fighting station is leaking continuously.","LSA / FFA","Eng. / Strg. Comp.","Equipment Related","","","","","Chnaged safety valve with spare received.","2020-09-30T23:59:35","MOJO200155","Completed","2020-09-29T23:59:35","Yes","No","No","Internal","This defect is from time of takeover, trust it has been rectified. Update job accordingly."]
[null,null,null,7580,null,"93_Tue Feb 12 2019 10:50:43 GMT+0000 (Coordinated Universal Time)","2019-08-20T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Yard supplied many cooking apparatus inoperational in galley. Only hot plates, one small kneader & one baking oven shelf working.","Miscellaneous","MLC Related","Equipment Related","","","","","Hot plates supplied and installed in location.","2020-06-30T23:59:35","","Completed","2020-05-13T23:59:35","Yes","No","No","Internal","Will be supplied at next convenient port as delivery time is 27 days. This defect has been attended by ship staff after receipt of spare during docking so Date Recorded has to be amended  accordingly."]
[null,null,null,7581,null,"93_Tue Feb 12 2019 11:24:58 GMT+0000 (Coordinated Universal Time)","2019-08-20T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Water leaking from Main engine jacket temperature controler 3-way valve spindle. ","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","O rings renewed , leak rectifed .","2020-03-31T23:59:35","","Completed","2020-04-06T23:59:35","No","No","No","Internal"]
[null,null,null,7673,null,"93_Mon Dec 02 2019 10:53:17 GMT+0000 (Coordinated Universal Time)","2019-08-20T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Main Engine oil mist detector was showing error E014 which is negative pressure/air flow too low & the alarm is kept in off-scan condition.The alarm is in offscan condition. ","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Same was rectified by ship staff after take over","2020-01-31T23:59:35","015E/19","Completed","2019-11-10T23:59:35","Yes","No","No","Internal"]
[null,null,null,7582,null,"93_Tue Feb 12 2019 11:26:24 GMT+0000 (Coordinated Universal Time)","2019-08-21T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Fwd winches & windlass power pack, temp. control sensor by-passed to avoid frequent overheating trip. ","Deck - Mooring Machinery","Mooring","Equipment Related","","","","","Fwd winches & windlass power pack, temp. control sensor working satisfactory and cooling water is able to control the temperature of the power pack.","2020-03-31T23:59:35","","Completed","2020-04-08T23:59:35","Yes","No","No","Internal"]
[null,null,null,7583,null,"93_Tue Feb 12 2019 11:27:53 GMT+0000 (Coordinated Universal Time)","2019-08-21T23:59:35","Defect","Ship Staff","Ship Staff Insp.","All W/T door dogs on deck not free","Miscellaneous","Structural Condn. / WT integrity ","Equipment Related","","","",""," All W/T door dogs  overhauled.","2020-07-31T23:59:35","","Completed","2020-06-06T23:59:35","Yes","No","No","Internal","This observation is almost 10 months old, confirm it has been taken care. Update job status accordingly as still reflecting NOT STARTED."]
[null,null,null,7584,null,"93_Tue Feb 12 2019 11:29:46 GMT+0000 (Coordinated Universal Time)","2019-08-21T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Fire & G/S pump alone not efficient for ballast tank eductor operation. Onboard C/O using 02 pumps for WBT final eduction","Elect. Mach. & Equip.","Cargo / Ballast Systems","Equipment Related","","","","","Eductors renewed in dry dock and efficiency checked in richard's bay while loading. Single pump used for educting and found satisfactory.","2020-03-31T23:59:35","","Completed","2020-05-23T23:59:35","Yes","No","No","Internal"]
[null,null,null,7585,null,"93_Tue Feb 12 2019 11:31:48 GMT+0000 (Coordinated Universal Time)","2019-08-21T23:59:35","Defect","Ship Staff","Ship Staff Insp.","All remote sounding gauges, draft gauges in ship's office not operational. ","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","Remote gauges were attended by the shore technician from IMA.","2020-03-31T23:59:35","","Completed","2020-04-13T23:59:35","Yes","No","No","Internal"]
[null,null,null,7586,null,"93_Tue Feb 12 2019 11:33:09 GMT+0000 (Coordinated Universal Time)","2019-08-21T23:59:35","Defect","Ship Staff","Ship Staff Insp.","No.03 WBT (P) remote shut indication light on ballast panel malfuntioning. Sensor to be checked at the actual v/v body in pipe duct. ., 2 REMOTE CONTROL VVs (REPORT FM KUIDA TECHNICIAN DD 05/04/20), P.O RAISED","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","","","","","No.3 WBT (P) remote open/shut indication sensor replaced with the spare recieved and tried out found working satisfactory.","2021-01-25T23:59:35","MOJO200093","Completed","2021-01-09T23:59:35","No","No","No","Internal","Waiting for owners approval."]
[null,null,null,7588,null,"93_Tue Feb 12 2019 11:36:58 GMT+0000 (Coordinated Universal Time)","2019-08-21T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Both lifeboat - falls, self lowering wires & gripes due for renewal in next DD. ","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","Lifeboat falls, self lowering wire and Gripes renewed .","2020-03-31T23:59:35","","Completed","2020-05-11T23:59:35","Yes","No","No","Internal"]
[null,null,null,7589,null,"93_Mon Dec 02 2019 11:41:30 GMT+0000 (Coordinated Universal Time)","2019-08-21T23:59:35","Defect","Ship Staff","Ship Staff Insp.","All 3 A/E's are capable of taking only 340kW and below  with exhaust temperatures at around 480 degree celcius.(rated capacity 730 kW)resulting in breakage of exhaust valves\n\nSUSPECT: wrong timing and use of non genuine spares like inlet valve,s,exhaust valves,fuel valve nozzles,coolers and the turbochargers.Also appears that the lube oil used are in excess of 2000 running hours and not purified. ","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","All the three AEs overhauled in DD. Performance test carried out at 75% , found satifactory.","2020-03-31T23:59:35","016E/19","Completed","2020-03-22T23:59:35","Yes","No","No","Internal"]
[null,null,null,7590,null,"93_Tue Feb 12 2019 11:43:47 GMT+0000 (Coordinated Universal Time)","2019-08-21T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Bilge fire & GS pump overboard valve gland leaking","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","Gland Packing renewed , leak rectified","2020-01-31T23:59:35","","Completed","2020-01-18T23:59:35","No","No","No","Internal"]
[null,null,null,7591,null,"93_Tue Feb 12 2019 11:46:14 GMT+0000 (Coordinated Universal Time)","2019-08-21T23:59:35","Defect","Ship Staff","Ship Staff Insp.","No.3 HFO bunker tank Stbd, minor fuel oil leakage from the tank gauging system sensor","E/R - Aux. Engine","MARPOL Related","Equipment Related","","","","","Gasket renewed, leak rectified","2020-01-31T23:59:35","","Completed","2020-01-15T23:59:35","No","No","No","Internal"]
[null,null,null,7592,null,"93_Tue Feb 12 2019 11:47:36 GMT+0000 (Coordinated Universal Time)","2019-08-21T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Main engine unit No.2 cylinder oil lubricator inlet line Y-filter leaking form the plug","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Gasket renewed, leak rectifed","2020-01-31T23:59:35","","Completed","2020-01-08T23:59:35","No","No","No","Internal"]
[null,null,null,7593,null,"93_Tue Feb 12 2019 11:52:16 GMT+0000 (Coordinated Universal Time)","2019-08-21T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Loadicator Computer is 15 yrs old. Same should be renewed to a newer computer & get Class approved. ","Miscellaneous","Cargo / Ballast Systems","Equipment Related","","","","","Job cancelled by the owners.","2020-03-31T23:59:35","","Completed","2020-04-13T23:59:35","No","No","No","Internal"]
[null,null,null,7594,null,"93_Tue Feb 12 2019 11:54:11 GMT+0000 (Coordinated Universal Time)","2019-08-21T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Both sides bridge wing, bridge front glass & its frame not clear & corroded & wasted respectively ","Navigation - Others","Navigation","Equipment Related","","","","","Glass and frames of portholes were attended in DD. Frames renewed and glass cleaned thoroughly.","2020-03-31T23:59:35","","Completed","2020-03-20T23:59:35","Yes","No","No","Internal"]
[null,null,null,7595,null,"93_Tue Feb 12 2019 11:56:09 GMT+0000 (Coordinated Universal Time)","2019-08-21T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Fwd winches & windlass power pack have drip hydraulic oil leakage from its pipe. ","Deck - Mooring Machinery","Mooring","Equipment Related","","","","","Leakage rectified.","2020-03-31T23:59:35","","Completed","2020-05-15T23:59:35","No","No","No","Internal"]
[null,null,null,7596,null,"93_Mon Dec 02 2019 11:50:50 GMT+0000 (Coordinated Universal Time)","2019-08-21T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Cargo hold bilge eductor & ballast tank eductor were with doubler plate & jubilee clip repairs respectively, Now the doubler plate has been replaced with soft patch repair & some hot repair. ","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","","","","","Both eductors renewed in DD by Ship's staff.","2020-03-31T23:59:35","34DD/19","Completed","2020-04-11T23:59:35","Yes","No","No","Internal"]
[null,null,null,7597,null,"93_Tue Feb 12 2019 11:57:53 GMT+0000 (Coordinated Universal Time)","2019-08-21T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Vessel unable to compact garbage volume & hence leading to garbage accumulation onboard. ","Miscellaneous","MARPOL Related","Equipment Related","","","","","Vessel received Garbage compactor in DD and compaction is done regularly.","2020-03-31T23:59:35","","Completed","2020-04-20T23:59:35","Yes","No","No","Internal"]
[null,null,null,7598,null,"93_Tue Feb 12 2019 11:59:53 GMT+0000 (Coordinated Universal Time)","2019-08-21T23:59:35","Defect","Ship Staff","MLC Audit","All cabin portholes on accommodation super structure are in poor condition & on outside show heavy rusting on the edges thus causing water ingress. ","Accommodation","MLC Related","Equipment Related","","","","","All porthole edges thoroughly derusted & sealed properly & then primered & painted. Portholes frames were sealed with silicon by attending team in DD.","2020-03-31T23:59:35","","Completed","2020-03-20T23:59:35","Yes","No","No","Internal"]
[null,null,null,7599,null,"93_Tue Feb 12 2019 12:01:24 GMT+0000 (Coordinated Universal Time)","2019-08-21T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Bridge Wings underside rusted at many unaccessible places. ","Accommodation","Structural Condn. / WT integrity ","Equipment Related","","","","","Both Bridge wing underside derusted, and painted with two coats primer and full finish coat in DD by Ship's staff.","2020-03-31T23:59:35","","Completed","2020-03-04T23:59:35","Yes","No","No","Internal"]
[null,null,null,7600,null,"93_Tue Feb 12 2019 12:02:54 GMT+0000 (Coordinated Universal Time)","2019-08-21T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Emergency generator radiator damaged badly and water leaking. ","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Radiator of the emergency generator renewed with new spare, the generator tried out , found working satisfactory with no leaks.","2020-01-31T23:59:35","","Completed","2019-12-16T23:59:35","No","No","No","Internal"]
[null,null,null,7601,null,"93_Tue Feb 12 2019 12:04:43 GMT+0000 (Coordinated Universal Time)","2019-08-21T23:59:35","Defect","Ship Staff","Ship Staff Insp.","No.1 HFO bunker tank port & stbd and Fuel oil overflow tank level gauge defective.","Hull & Tanks","Eng. / Strg. Comp.","Equipment Related","","","","","Sensor installed and cables layed. Level transmitters are working now. ","2020-01-15T23:59:35","MOJO200098","Completed","2020-12-04T23:59:35","No","No","No","Internal","Spares will be supplied at next convenient port"]
[null,null,null,7602,null,"93_Tue Feb 12 2019 12:06:46 GMT+0000 (Coordinated Universal Time)","2019-08-21T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Rescue boat(port) battery expiring on May 2020. ","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","Battery renewed with new spare battery.","2020-03-31T23:59:35","","Completed","2020-04-05T23:59:35","No","No","No","Internal"]
[null,null,null,8952,null,"93_Tue Feb 12 2019 11:50:50 GMT+0000 (Coordinated Universal Time)","2019-08-21T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Cargo hold bilge eductor & ballast tank eductor were with doubler plate & jubilee clip repairs respectively, Now the doubler plate has been replaced with soft patch repair & some hot repair. ","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","","","","","Both Eductors renewed in DD by ship's staff.","2020-03-31T23:59:35","","Completed","2020-04-11T23:59:35","Yes","No","No","Internal"]
[null,null,null,7674,null,"93_Mon Dec 02 2019 11:49:26 GMT+0000 (Coordinated Universal Time)","2019-08-21T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Topping up compressor is not being used, as it is not building up pressure","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","Ship staff has put the compressor in use after take over.","2020-01-31T23:59:35","","Completed","2019-11-15T23:59:35","No","No","No","Internal"]
[null,null,null,7687,null,"93_Tue Mar 12 2019 07:53:21 GMT+0000 (Coordinated Universal Time)","2019-08-22T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Vacuum toilet pump No.1 minor leakage. ","E/R - Aux. Mach.","MLC Related","Equipment Related","","","","","O ring of the casing renewed, leak rectified.","2020-01-31T23:59:35","","Completed","2019-12-13T23:59:35","No","No","No","Internal"]
[null,null,null,7688,null,"93_Tue Dec 03 2019 07:55:32 GMT+0000 (Coordinated Universal Time)","2019-08-22T23:59:35","Defect","Ship Staff","Ship Staff Insp.","FWG feed water line chemical dosing pump not running","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","",""," The chemical dosing pump tried out and put in use, found working satisfactory","2020-01-31T23:59:35","","Completed","2019-12-10T23:59:35","No","No","No","Internal"]
[null,null,null,7693,null,"93_Tue Dec 03 2019 06:30:55 GMT+0000 (Coordinated Universal Time)","2019-08-22T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Master's cabin entrance door curtain in poor condition. ","Miscellaneous","MLC Related","Equipment Related","","","","","Replaced with new one.","2020-01-31T23:59:35","001D/19","Completed","2020-01-05T23:59:35","No","No","No","Internal"]
[null,null,null,7603,null,"93_Tue Mar 12 2019 06:14:55 GMT+0000 (Coordinated Universal Time)","2019-08-22T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Excessive condemned material in forecastle store. .","Miscellaneous","MARPOL Related","Equipment Related","","","","","Condemned material landed at Jin Hai ship yard.","2020-03-31T23:59:35","","Completed","2020-04-13T23:59:35","No","No","No","Internal"]
[null,null,null,7604,null,"93_Tue Mar 12 2019 06:22:19 GMT+0000 (Coordinated Universal Time)","2019-08-22T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Vessel has 03 pcs pneumatic de-mucking davits in defunct condition. Same to be made operational.","Miscellaneous","Cargo / Ballast Systems","Equipment Related","","","","","2 De-mucking winch are operational and vessel is using them for cargo hold cleaning.","2020-08-31T23:59:35","","Completed","2020-04-13T23:59:35","Yes","No","No","Internal","This observation was raised in 2019 during takeover, revert what vessel has found reason for not operation of it ."]
[null,null,null,7605,null,"93_Tue Mar 12 2019 06:24:47 GMT+0000 (Coordinated Universal Time)","2019-08-22T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Fwd P side Windlass motor gear engaging hydraulic mechanism has been removed from place & manual engagament used. ","Deck - Mooring Machinery","Mooring","Equipment Related","","","","","As per Owners instructions, the gear engaging mechanism is operational and does not require any modification. Hence job is cancelled.","2020-03-31T23:59:35","","Completed","2020-01-10T23:59:35","Yes","No","No","Internal"]
[null,null,null,7606,null,"93_Tue Mar 12 2019 06:26:03 GMT+0000 (Coordinated Universal Time)","2019-08-22T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Fwd S side Windlass motor gear engaging hydraulic mechanism full corroded & about to break anytime. ","Deck - Mooring Machinery","Mooring","Equipment Related","","","","","As per Owners instructions, the gear engaging mechanism is operational and does not require any modification. Hence job is cancelled.","2020-01-31T23:59:35","","Completed","2020-01-10T23:59:35","Yes","No","No","Internal"]
[null,null,null,7607,null,"93_Tue Mar 12 2019 06:27:59 GMT+0000 (Coordinated Universal Time)","2019-08-22T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Fwd & Midship draft guage hydraulic purge v/v looks poorly maintained","Cargo Mach.,Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","","","","","Gauges attended in DD by technician and are operational. The purge valve maintained in DD.","2020-03-31T23:59:35","","Completed","2020-03-30T23:59:35","Yes","No","No","Internal"]
[null,null,null,7608,null,"93_Tue Mar 12 2019 06:29:22 GMT+0000 (Coordinated Universal Time)","2019-08-22T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Both FWTks & DWTk cleaning & washing not done in the last 06 months. ","Hull & Tanks","MLC Related","Equipment Related","","","","","All fresh water tanks and Drinking water tank cleaned in Dry dock by ship's crew..","2020-03-31T23:59:35","","Completed","2020-03-20T23:59:35","Yes","No","No","Internal"]
[null,null,null,7609,null,"93_Tue Mar 12 2019 06:33:14 GMT+0000 (Coordinated Universal Time)","2019-08-22T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Atmospheric condensor 14 Nos of tubes has been plugged. ","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","Complete atmospheric condensor renewed","2020-03-31T23:59:35","012E/19","Completed","2020-02-19T23:59:35","No","No","No","Internal"]
[null,null,null,7610,null,"93_Tue Mar 12 2019 06:35:20 GMT+0000 (Coordinated Universal Time)","2019-08-22T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Boiler feed water controller erratic and leaking from the gland.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","The gland leak rectified","2020-03-31T23:59:35","","Completed","2020-03-08T23:59:35","No","No","No","Internal"]
[null,null,null,7611,null,"93_Tue Mar 12 2019 06:38:53 GMT+0000 (Coordinated Universal Time)","2019-08-22T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Main Engine unit no.2,3 & 6 minor fuel oil leakage from shock absorber flange","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","All units fuel pump shock absorber oveerhauled and fitted with new gaskets, leaks rectified.","2020-03-31T23:59:35","","Completed","2020-04-02T23:59:35","No","No","No","Internal"]
[null,null,null,7612,null,"93_Tue Mar 12 2019 06:45:15 GMT+0000 (Coordinated Universal Time)","2019-08-22T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Main engine unit no.6  minor fuel oil leakage from aft high pressure pipe. ","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","High pressure pipe renewed.","2020-03-31T23:59:35","","Completed","2020-03-18T23:59:35","No","No","No","Internal"]
[null,null,null,7613,null,"93_Tue Mar 12 2019 06:47:01 GMT+0000 (Coordinated Universal Time)","2019-08-22T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Fwd Liferaft launching instructions poster in poor condition. ","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","Replaced with new one.","2020-01-31T23:59:35","","Completed","2020-01-02T23:59:35","No","No","No","Internal"]
[null,null,null,7614,null,"93_Tue Mar 12 2019 06:49:17 GMT+0000 (Coordinated Universal Time)","2019-08-22T23:59:35","Defect","Ship Staff","Ship Staff Insp.","All hatch cover opening chain drawing hydraulic motor open to shipping seas & thus prone to heavy seas & water damage.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","Owners did not approve the job.","2020-03-31T23:59:35","","Completed","2020-04-13T23:59:35","Yes","No","No","Internal"]
[null,null,null,7615,null,"93_Tue Mar 12 2019 07:48:12 GMT+0000 (Coordinated Universal Time)","2019-08-22T23:59:35","Defect","Ship Staff","Ship Staff Insp.","WBTks remote hydraulic v/v operating power pack pumps always kept 'ON' & pumps running continuously to maintain pressure. ","Elect. Mach. & Equip.","Cargo / Ballast Systems","Equipment Related","","","","","After investigation, the pumps need to be kept on only during the period of operation and hence is being used accordingly.","2020-01-31T23:59:35","","Completed","2020-01-24T23:59:35","No","No","No","Internal"]
[null,null,null,7616,null,"93_Tue Mar 12 2019 07:50:03 GMT+0000 (Coordinated Universal Time)","2019-08-22T23:59:35","Defect","Ship Staff","Ship Staff Insp.","All CH entrance booby hatches to be legibly stencilled following - \"Restricted Area, No unauthorized Access / Caution: Danger of Oxygen depletion\".","Hull & Tanks","Cargo / Ballast Systems","Equipment Related","","","","","stencilling completed","2021-01-31T23:59:35","","Completed","2020-12-16T23:59:35","No","No","No","Internal",""]
[null,null,null,7617,null,"93_Tue Mar 12 2019 07:56:56 GMT+0000 (Coordinated Universal Time)","2019-08-22T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Main engine unit no.3 aft fuel injector leaking. ","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Injector renewed with spare overhauled injector.The engine tried out , found no leaks","2020-01-31T23:59:35","","Completed","2020-01-02T23:59:35","No","No","No","Internal"]
[null,null,null,8953,null,"93_Tue Mar 12 2019 07:55:32 GMT+0000 (Coordinated Universal Time)","2019-08-22T23:59:35","Defect","Ship Staff","Ship Staff Insp.","FWG feed water line chemical dosing pump not running","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","",""," The chemical dosing pump inspected and put in use, found working satisfactory.","2020-01-31T23:59:35","","Completed","2019-12-10T23:59:35","No","No","No","Internal"]
[null,null,null,7675,null,"93_Tue Dec 03 2019 06:13:11 GMT+0000 (Coordinated Universal Time)","2019-08-22T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Overside painting stage is in poor condition. Bos'n chair with hook also not available onboard. ","Miscellaneous","General Appearance","Equipment Related","","","","","Received at Xiamen.","2020-01-31T23:59:35","008D/19","Completed","2019-11-08T23:59:35","No","No","No","Internal"]
[null,null,null,7676,null,"93_Tue Dec 03 2019 07:51:45 GMT+0000 (Coordinated Universal Time)","2019-08-22T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Helicopter Landing FFE- Fireman's Outfit Suit (02 pcs) completely worn out, helmets broken & unwearable. ","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","Received at Xiamen","2020-01-31T23:59:35","","Completed","2019-11-08T23:59:35","No","No","No","Internal"]
[null,null,null,7618,null,"93_Tue Mar 12 2019 07:59:22 GMT+0000 (Coordinated Universal Time)","2019-08-24T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Main engine unit no.3 fwd stbd cooling water connection pipe leaking","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","O rings renewed , leak rectified","2020-03-31T23:59:35","","Completed","2020-03-18T23:59:35","No","No","No","Internal"]
[null,null,null,7619,null,"93_Tue Mar 12 2019 08:01:02 GMT+0000 (Coordinated Universal Time)","2019-08-24T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Main engine camshaft lube oil inlet low pressure shutdown broken. Alarm showing in Safety system unit and alarm monitor. ","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Card on the SSU panel renewed, broken alarm found normal","2020-03-31T23:59:35","","Completed","2020-03-18T23:59:35","No","No","No","Internal"]
[null,null,null,7620,null,"93_Tue Mar 12 2019 08:03:04 GMT+0000 (Coordinated Universal Time)","2019-08-24T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Main Engine Running Hour meter not working","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","vessel has connected the new recieved main Engine Running Hour meter after modifying the connection circuit and the Running Hour counter is operational now.","2020-09-15T23:59:35","","Completed","2020-09-08T23:59:35","No","No","No","Internal","PO will be supplied at next convenient port."]
[null,null,null,7692,null,"93_Tue Mar 12 2019 08:07:37 GMT+0000 (Coordinated Universal Time)","2019-08-26T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Fireman's outfit suit & SCBAs visor in Fire Station looks worn out. One Safety helmet visor is missing. ","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","New Fireman's outfit & SCBA visors to be requisitioned along with one safety helmet with visor & neck protection","2020-01-31T23:59:35","004D/19","Completed","2019-11-30T23:59:35","No","No","No","Internal"]
[null,null,null,7621,null,"93_Tue Dec 03 2019 08:05:32 GMT+0000 (Coordinated Universal Time)","2019-08-26T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Actual location of Fireman's outfit not in compliance with Ship's Fire Safety Plan. Ship's Fire Safety Plan modified as per ship's convenience. But not all are updated. ","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","Actual location of Fireman's outfit made in compliance with Fire Safety Plan.","2020-03-31T23:59:35","","Completed","2020-04-13T23:59:35","No","No","No","Internal"]
[null,null,null,8954,null,"93_Tue Dec 03 2019 08:07:37 GMT+0000 (Coordinated Universal Time)","2019-08-26T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Fireman's outfit suit & SCBAs visor in Fire Station looks worn out. One Safety helmet visor is missing. ","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","New Fireman's outfit & SCBA visors to be received along with one safety helmet with visor & neck protection","2020-03-31T23:59:35","004D/19","Completed","2020-04-13T23:59:35","No","No","No","Internal"]
[null,null,null,7677,null,"93_Tue Dec 03 2019 08:09:25 GMT+0000 (Coordinated Universal Time)","2019-08-26T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Spare foam liquid in Fire Station stored in unlabelled water bottles. ","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","Spare foam charges receive at Xiamen","2020-01-31T23:59:35","011D/19","Completed","2019-11-08T23:59:35","No","No","No","Internal"]
[null,null,null,7622,null,"93_Tue Mar 12 2019 08:14:21 GMT+0000 (Coordinated Universal Time)","2019-08-27T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Main engine exhaust pipe above the funnel exhaust platform welding is completely gone in fwd both port and stbd support frame. ","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Section of the plate cropped and new supports welded","2020-03-31T23:59:35","","Completed","2020-03-08T23:59:35","Yes","No","No","Internal"]
[null,null,null,7623,null,"93_Tue Mar 12 2019 08:15:51 GMT+0000 (Coordinated Universal Time)","2019-08-27T23:59:35","Defect","Ship Staff","Ship Staff Insp.","All 3 Aux Engine exhaust pipe above the funnel exhaust platform completely rusted and holed. ","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","The exhaust pipes of all the 3 Aux Engine above the funnel cropped and new pipes fitted and supports welded","2020-03-31T23:59:35","","Completed","2020-04-01T23:59:35","Yes","No","No","Internal"]
[null,null,null,7624,null,"93_Tue Mar 12 2019 08:17:49 GMT+0000 (Coordinated Universal Time)","2019-08-27T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Incinerator exhaust pipe above the funnel exhaust platform rusted. ","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Incinerator exhaust pipe cropped and new pipe fitted.","2020-03-31T23:59:35","","Completed","2020-03-08T23:59:35","Yes","No","No","Internal"]
[null,null,null,7625,null,"93_Tue Mar 12 2019 08:20:26 GMT+0000 (Coordinated Universal Time)","2019-08-27T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Funnel hatch cover completely rusted","Hull & Tanks","Eng. / Strg. Comp.","Equipment Related","","","","","The hatch cover renewed.","2020-03-31T23:59:35","","Completed","2020-03-08T23:59:35","Yes","No","No","Internal"]
[null,null,null,7626,null,"93_Tue Mar 12 2019 08:31:38 GMT+0000 (Coordinated Universal Time)","2019-08-27T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Sewage discharge pump delivery line two section of pipes is holed in many places. Need to renewe the pipe.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","The pipe renewed with newly fabricated pipe","2020-03-31T23:59:35","","Completed","2020-04-03T23:59:35","No","No","No","Internal"]
[null,null,null,7627,null,"93_Tue Mar 12 2019 08:33:16 GMT+0000 (Coordinated Universal Time)","2019-08-27T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Main engine unit No.1 port side FWD and AFT cooling water connection pipe minor leakage. ","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Cooling water connection O rings renewed , leak rectified","2020-03-31T23:59:35","","Completed","2020-03-18T23:59:35","No","No","No","Internal"]
[null,null,null,7628,null,"93_Tue Mar 12 2019 08:50:35 GMT+0000 (Coordinated Universal Time)","2019-08-27T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Main engine fuel oil auto filter running hour meter is not working.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Job captured in duplication previously.","2020-06-30T23:59:35","","Completed","2020-06-07T23:59:35","No","No","No","Internal","This observation is captured two times, delete one observation."]
[null,null,null,7679,null,"93_Tue Dec 03 2019 08:12:22 GMT+0000 (Coordinated Universal Time)","2019-08-27T23:59:35","Defect","Ship Staff","Ship Staff Insp.","VDR data never downloaded by ship staff.","Navigation - VDR / BNWAS","Navigation","Equipment Related","","","","","Data downloaded by shore technician during re-programming at Xiamen","2020-01-31T23:59:35","","Completed","2019-11-10T23:59:35","No","No","No","Internal"]
[null,null,null,7629,null,"93_Tue Mar 12 2019 08:52:43 GMT+0000 (Coordinated Universal Time)","2019-08-28T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Some W/T doors not sealing properly on closure. Also packing retaining channel seems corroded.","Accommodation","Structural Condn. / WT integrity ","Equipment Related","","","","","All W/T doors checked for proper sealing. Packing retaining channel derusted & painted. ","2020-08-15T23:59:35","","Completed","2020-07-30T23:59:35","No","No","No","Internal","Vsl to update job progress via weekly maintenance reports."]
[null,null,null,7630,null,"93_Tue Mar 12 2019 08:54:24 GMT+0000 (Coordinated Universal Time)","2019-08-28T23:59:35","Defect","Ship Staff","Ship Staff Insp.","All 03 embarkation ladders for both lifeboats & fwd liferafts, the shackle end thimble area & exposed ladder parts shows Sunrays / SW damage. .","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","New embarkation ladder received and other Embarkation ladders checked for wear & found in satisfactory condition.","2020-03-31T23:59:35","013D/19","Completed","2020-02-13T23:59:35","No","No","No","Internal"]
[null,null,null,7631,null,"93_Tue Mar 12 2019 08:56:50 GMT+0000 (Coordinated Universal Time)","2019-08-28T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Boiler fuel oil pump No.2 shaft seal leaking. ","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","Pump overhauled , seal renewed","2020-03-31T23:59:35","","Completed","2020-03-11T23:59:35","No","No","No","Internal"]
[null,null,null,7632,null,"93_Tue Mar 12 2019 09:00:41 GMT+0000 (Coordinated Universal Time)","2019-08-28T23:59:35","Defect","Ship Staff","Ship Staff Insp.","No.1 HFO Purifier Fuel oil leaking from the inlet/outlet pipe flange. ","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","The gaskets of the inlet and outlet pipe flanges renewed, leak rectified","2020-01-31T23:59:35","","Completed","2019-12-03T23:59:35","No","No","No","Internal"]
[null,null,null,7633,null,"93_Tue Mar 12 2019 09:04:37 GMT+0000 (Coordinated Universal Time)","2019-08-28T23:59:35","Defect","Ship Staff","Ship Staff Insp.","A/E No.3 lube oil inlet pipe to turbocharger leaking. ","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Turbocharger overhauled, O ring renewed, leak rectified","2020-03-31T23:59:35","","Completed","2020-03-25T23:59:35","No","No","No","Internal"]
[null,null,null,7634,null,"93_Tue Dec 03 2019 09:10:15 GMT+0000 (Coordinated Universal Time)","2019-08-28T23:59:35","Defect","Ship Staff","Ship Staff Insp.","A/E ACONICS PMS system need to check as A/E synchronizing is being done manually. .","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","AE ACONIS PMS tried out , all the three generators are able to take on load on auto","2019-11-30T23:59:35","","Completed","2019-11-20T23:59:35","No","No","No","Internal"]
[null,null,null,7689,null,"93_Tue Mar 12 2019 09:20:59 GMT+0000 (Coordinated Universal Time)","2019-08-29T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Boiler burner unit attached fuel oil pump leaking from shaft seal. ","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","The fuel pump renewed with new spare pump, leak rectified","2020-01-31T23:59:35","20000000000000000000","Completed","2019-12-01T23:59:35","No","No","No","Internal"]
[null,null,null,7635,null,"93_Tue Mar 12 2019 09:18:51 GMT+0000 (Coordinated Universal Time)","2019-08-29T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Fresh water expansion tank have some oil trace, A/E fuel injector is being cooled by fresh water.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Upon investigation found, Unit #2 of AE 3 was leaking through the noozle cooing line and oil finding its way to the expansion tank. Chemical 'SEACLEAN' was added as per instructions to collect the oil from the line and thereby collecing at the expansion tank.On 29/09/2020&26/10/2020, FW expansion tank partially drained till low level alarm and replenished with fresh water. Vessel to monitor further and replinesh as necessary clean fresh water.","2020-12-31T23:59:35","","Completed","2020-12-04T23:59:35","No","No","No","Internal","Vsl to update job progress by mail ."]
[null,null,null,7636,null,"93_Tue Mar 12 2019 09:24:31 GMT+0000 (Coordinated Universal Time)","2019-08-29T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Sea chest both Low & High and Cooling sea water overboard valves have remote operating option(From 2nd Deck) but not working. ","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Hydraulic oil topped up,tried out the remote operation , operating satisfactory.","2020-01-31T23:59:35","","Completed","2019-12-03T23:59:35","No","No","No","Internal"]
[null,null,null,8955,null,"93_Tue Dec 03 2019 09:20:59 GMT+0000 (Coordinated Universal Time)","2019-08-29T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Boiler burner unit attached fuel oil pump leaking from shaft seal. ","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","The fuel oil pump renewed with new spare pump, tried out, working satisfactory with no leaks","2020-01-31T23:59:35","20000000000000000000","Completed","2020-12-01T23:59:35","No","No","No","Internal"]
[null,null,null,7678,null,"93_Tue Dec 03 2019 09:16:17 GMT+0000 (Coordinated Universal Time)","2019-08-29T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Portable extinguishers spare charges not in compliance with Ship's Fire Safety Plan or even SOLAS or flag requirement. ","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","Spare charges for portable extinguishers received at Xiamen","2019-11-30T23:59:35","","Completed","2019-11-08T23:59:35","No","No","No","Internal"]
[null,null,null,7637,null,"93_Tue Mar 12 2019 09:27:12 GMT+0000 (Coordinated Universal Time)","2019-08-30T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Bridge wings - Anti skid walking mats in worn out condition. ","Accommodation","General Appearance","Equipment Related","","","","","New mats installed in location on bridge wings.","2020-03-31T23:59:35","","Completed","2020-06-03T23:59:35","Yes","No","No","Internal"]
[null,null,null,7680,null,"93_Tue Dec 03 2019 09:32:14 GMT+0000 (Coordinated Universal Time)","2019-09-02T23:59:35","Defect","Ship Staff","Ship Staff Insp.","SI lights on lifebuoys on deck looks worn out. ","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","New SI lights received at Xiamen","2020-01-31T23:59:35","011D/19","Completed","2019-11-08T23:59:35","No","No","No","Internal"]
[null,null,null,7681,null,"93_Tue Dec 03 2019 09:34:49 GMT+0000 (Coordinated Universal Time)","2019-09-02T23:59:35","Defect","Ship Staff","Ship Staff Insp.","EPIRB HRU expiring in Nov 2019. ","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","New HRU ordered & installed.","2019-11-05T23:59:35","011D/19","Completed","2019-11-10T23:59:35","No","No","No","Internal"]
[null,null,null,7682,null,"93_Tue Dec 03 2019 09:37:02 GMT+0000 (Coordinated Universal Time)","2019-09-02T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Helicopter FFE foam concentrate stock is manufactured 2013 / 2014. More than 05 years old. ","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","Replaced with new stock, received at Xiamen.","2019-11-30T23:59:35","011D/19","Completed","2019-11-08T23:59:35","No","No","No","Internal"]
[null,null,null,7691,null,"93_Tue Dec 03 2019 09:39:49 GMT+0000 (Coordinated Universal Time)","2019-09-02T23:59:35","Defect","Ship Staff","Ship Staff Insp.","No.2 main air compressor oil is getting emulsification. ","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","The main air compressor crankcase inspected , find no leaks , the sump oil drained and replenished with fresh oil. ","2019-12-30T23:59:35","","Completed","2019-12-03T23:59:35","No","No","No","Internal"]
[null,null,null,7638,null,"93_Tue Mar 12 2019 09:29:34 GMT+0000 (Coordinated Universal Time)","2019-09-02T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Vessel hawse pipes have no covering arrangement on forecastle deck for anti pilferage measure. Hawse pipe covers stowed in FPK store. ","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","Equipment Related","","","","","New Hawse pipe covers installed on forecastle deck & put in use.","2020-03-31T23:59:35","","Completed","2020-05-15T23:59:35","No","No","No","Internal"]
[null,null,null,7639,null,"93_Tue Mar 12 2019 09:42:44 GMT+0000 (Coordinated Universal Time)","2019-09-02T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Soft patch in STBD grey water overboard pipe line in bottom platform. ","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Pipe renewed at Dry Dock","2020-03-31T23:59:35","","Completed","2020-02-24T23:59:35","No","No","No","Internal"]
[null,null,null,8956,null,"93_Tue Mar 12 2019 09:39:49 GMT+0000 (Coordinated Universal Time)","2019-09-02T23:59:35","Defect","Ship Staff","Ship Staff Insp.","No.2 main air compressor oil is getting emulsification. ","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","The cooler gasket renewed, the crankcase inspected, the old oil drained and replenished with fresh oil.","2019-12-30T23:59:35","","Completed","2019-12-03T23:59:35","No","No","No","Internal"]
[null,null,null,7541,null,"93_Tue Mar 12 2019 09:53:04 GMT+0000 (Coordinated Universal Time)","2019-09-04T23:59:35","Defect","Ship Staff","Ship Staff Insp.","A/E lube oil settling tank is filled with 8.45 m3 of sludge and water. ","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","The contents of the tank disposed to barge, tank cleaned.","2020-01-31T23:59:35","","Completed","2019-12-26T23:59:35","No","No","No","Internal"]
[null,null,null,7640,null,"93_Tue Mar 12 2019 09:50:42 GMT+0000 (Coordinated Universal Time)","2019-09-04T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Steam pipe in purifier room is leaking from the flange. ","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Gasket renewed , leak rectified","2020-03-31T23:59:35","","Completed","2020-02-12T23:59:35","No","No","No","Internal"]
[null,null,null,7641,null,"93_Tue Mar 12 2019 09:55:25 GMT+0000 (Coordinated Universal Time)","2019-09-04T23:59:35","Defect","Ship Staff","Ship Staff Insp.","M/E lube oil settling tank is filled with 6.5 m3 of used oil. ","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","The contents of the tank disposed to barge, the tank cleaned","2020-01-31T23:59:35","","Completed","2019-12-26T23:59:35","No","No","No","Internal"]
[null,null,null,7642,null,"93_Tue Mar 12 2019 10:00:30 GMT+0000 (Coordinated Universal Time)","2019-09-04T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Pressure and temperature gauges of various pumps not working. ","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Defective gauges renewed.","2020-01-31T23:59:35","011E/19","Completed","2020-03-26T23:59:35","No","No","No","Internal"]
[null,null,null,7669,null,"93_Tue Dec 03 2019 09:45:42 GMT+0000 (Coordinated Universal Time)","2019-09-04T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Understand from ship staff, vessel has water ingress issue from No.02 CH Tank top","Hull & Tanks","Cargo / Ballast Systems","Equipment Related","","","","","NO.2 CH tanktop repaired with insert plate in presence of class surveyor at Putian berth.","2020-01-31T23:59:35","","Completed","2019-11-01T23:59:35","No","No","No","Internal"]
[null,null,null,7670,null,"93_Tue Mar 12 2019 09:48:54 GMT+0000 (Coordinated Universal Time)","2019-09-04T23:59:35","Defect","Ship Staff","Ship Staff Insp.","All Garbage collection receptacles to be colour coded as per Company GMP","Miscellaneous","MARPOL Related","Equipment Related","","","","","Garbage Receptacles colour coded as per the Garbage Management Plan","2020-01-31T23:59:35","","Completed","2019-12-03T23:59:35","No","No","No","Internal"]
[null,null,null,7643,null,"93_Tue Mar 12 2019 10:02:35 GMT+0000 (Coordinated Universal Time)","2019-09-09T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Both lifeboats, fwd & aft hooks engaged & locked position yellow marking is missing. ","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","Both Lifeboat hooks marked as per instructions.","2020-03-05T23:59:35","","Completed","2020-02-24T23:59:35","No","No","No","Internal"]
[null,null,null,7644,null,"93_Tue Mar 12 2019 10:04:14 GMT+0000 (Coordinated Universal Time)","2019-09-10T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Both Boiler feed water pump discharge line holes repaired with soft patch","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","The feed water pump discharge lines renewed.","2020-03-31T23:59:35","","Completed","2020-02-24T23:59:35","No","No","No","Internal"]
[null,null,null,7645,null,"93_Tue Mar 12 2019 10:11:44 GMT+0000 (Coordinated Universal Time)","2019-09-10T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Oily bilge pump discharge line to OWS many places corroded and have trace of leakage. ","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","The entire discharge line from the Oily bilge pump to OWS renewed with newly fabricated pipe line.","2020-03-31T23:59:35","","Completed","2020-02-24T23:59:35","No","No","No","Internal"]
[null,null,null,7646,null,"93_Tue Mar 12 2019 10:14:14 GMT+0000 (Coordinated Universal Time)","2019-09-10T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Oxygen cylinder room closing valve have soft patch. .","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","The Oxygen Cylinder room closing valve renewed.","2020-03-31T23:59:35","009E/19","Completed","2020-03-25T23:59:35","No","No","No","Internal"]
[null,null,null,7647,null,"93_Tue Dec 03 2019 10:31:12 GMT+0000 (Coordinated Universal Time)","2019-10-18T23:59:35","Defect","Ship Staff","Ship Staff Insp.","No.03 hatch cover chain drawing hydraulic motor in not working condition & lying defunct.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","Existing hydraulic Drawing chain motor was overhauled and bearing , bushes and seal renewed by the Vendor. No.3 Hatch cover motor is working satisfactory.","2020-03-31T23:59:35","017E/19","Completed","2020-04-12T23:59:35","No","No","No","Internal"]
[null,null,null,7648,null,"93_Tue Mar 12 2019 10:33:09 GMT+0000 (Coordinated Universal Time)","2019-10-26T23:59:35","Defect","Ship Staff","Ship Staff Insp.","All hatch cover chain drawing hydraulic motors to be overhauled. (09 pcs) ","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","All hatch cover hydraulic drawing chain motoroverhauled, bearings, bushes and seals renewed as required by the ship yard.","2020-03-31T23:59:35","","Completed","2020-04-12T23:59:35","Yes","No","No","Internal"]
[null,null,null,7683,null,"93_Tue Dec 03 2019 10:45:09 GMT+0000 (Coordinated Universal Time)","2019-10-31T23:59:35","Defect","Ship Staff","Ship Staff Insp.","No.02 CH straight ladder bottom platform is damaged during present discharging operation at Luoyu port. ","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","Repaired by shore staff at Putian berth","2020-11-05T23:59:35","","Completed","2019-11-01T23:59:35","No","No","No","Internal"]
[null,null,null,7649,null,"93_Tue Mar 12 2019 10:35:18 GMT+0000 (Coordinated Universal Time)","2019-10-31T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Fire & G/S pump No.2 leaking from shaft seal. .","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","The Pump overhauled, the mechanical seal renewed.","2020-03-31T23:59:35","","Completed","2020-03-19T23:59:35","No","No","No","Internal"]
[null,null,null,7650,null,"93_Tue Mar 12 2019 10:37:26 GMT+0000 (Coordinated Universal Time)","2019-10-31T23:59:35","Defect","Ship Staff","Ship Staff Insp.","A/E fuel oil heater found slightly leaking from the end cover flange. ","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","The heater cleaned and pressure tested , the gasket renewed, leak rectified.","2020-01-31T23:59:35","","Completed","2020-02-21T23:59:35","No","No","No","Internal"]
[null,null,null,7651,null,"93_Tue Mar 12 2019 10:39:44 GMT+0000 (Coordinated Universal Time)","2019-10-31T23:59:35","Defect","Ship Staff","Ship Staff Insp.","FWG observed to be producing only 10 to 12 MT/day                   (capacity :- 25 MT) ","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Evaporatorcleaned , the choked tubes cleared and pressure tested. The condenser and the demister cleaned.","2020-03-31T23:59:35","","Completed","2020-03-28T23:59:35","Yes","No","No","Internal"]
[null,null,null,7652,null,"93_Tue Mar 12 2019 10:42:12 GMT+0000 (Coordinated Universal Time)","2019-10-31T23:59:35","Defect","Ship Staff","Ship Staff Insp.","All stained steam laggings in purifier room/Generators/Boilers/ME/General laggings in Engine Room. ","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","All the stained laggings renewed.","2020-03-31T23:59:35","","Completed","2020-04-05T23:59:35","Yes","No","No","Internal"]
[null,null,null,7684,null,"93_Tue Dec 03 2019 10:54:26 GMT+0000 (Coordinated Universal Time)","2019-11-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Blr feed water salinometer in alarm condition. ","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","Rectified by ship staff after take over","2020-01-31T23:59:35","","Completed","2019-11-17T23:59:35","No","No","No","Internal"]
[null,null,null,7685,null,"93_Tue Mar 12 2019 11:29:39 GMT+0000 (Coordinated Universal Time)","2019-11-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Vessel has no spare mooring ropes, other than those on drums. ","Deck - Mooring Machinery","Mooring","Equipment Related","","","","","Vessel supplied with 02 spare mooring ropes at Xiamen","2020-11-05T23:59:35","012D/19","Completed","2019-11-08T23:59:35","No","No","No","Internal"]
[null,null,null,7686,null,"93_Tue Dec 03 2019 11:14:58 GMT+0000 (Coordinated Universal Time)","2019-11-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Emergency generator abnormal alarm existing/not in ready to start position. ","Critical Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","Inspected & rectified","2020-01-31T23:59:35","","Completed","2019-11-20T23:59:35","No","No","No","Internal"]
[null,null,null,7690,null,"93_Tue Dec 03 2019 11:13:14 GMT+0000 (Coordinated Universal Time)","2019-11-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","WMFF system in alarm condition/panel abnormal alarm. ","Critical Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","All the flame sensors and the smoke sensors of the WMFSS checked , the faulty smoke sensors renewed with new sensors and now the system is back to normal with no alarms in the panel","2020-01-31T23:59:35","","Completed","2019-12-08T23:59:35","No","No","No","Internal"]
[null,null,null,7653,null,"93_Tue Mar 12 2019 10:48:43 GMT+0000 (Coordinated Universal Time)","2019-11-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","All WB TSTs & DBTs onboard need thorough demucking, UT guaging & rerusting & painiting as required. ","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","Equipment Related","","","","","All ballast tanks UT gauging done by attending team and demucking cancelled by the Owners. Maintenance to be carried out in ballast tank on Owner's instructions.","2020-03-31T23:59:35","","Completed","2020-04-12T23:59:35","Yes","No","No","Internal"]
[null,null,null,7654,null,"93_Tue Mar 12 2019 10:52:24 GMT+0000 (Coordinated Universal Time)","2019-11-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","All lifting cranes & davit main wires + ancillary wires wires on board due for renewal in DD. (01 prov. Crane, 01 E/R o/h crane, 02 bunker davits, 02 gangways). ","Deck - Machinery","Structural Condn. / WT integrity ","Equipment Related","","","","","New wires received and installed in location. certificates updated in file.","2020-03-31T23:59:35","","Completed","2020-05-13T23:59:35","Yes","No","No","Internal"]
[null,null,null,7655,null,"93_Tue Mar 12 2019 10:56:11 GMT+0000 (Coordinated Universal Time)","2019-11-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Few  exhaust temperature guages for the AE are faulty and few are missing. ","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","The exhaust temperature guages of all the three AEs fitted with new temperature guages.","2020-03-31T23:59:35","","Completed","2020-03-22T23:59:35","No","No","No","Internal"]
[null,null,null,7656,null,"93_Tue Mar 12 2019 11:07:15 GMT+0000 (Coordinated Universal Time)","2019-11-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","ME fuel oil auto filter running hour meter not operational.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","ME fuel oil auto filter running hour meter changed with spare recieved.","2020-08-31T23:59:35","MOJO200102","Completed","2020-07-23T23:59:35","No","No","No","Internal","Spare will be supplied at next convenient port."]
[null,null,null,7657,null,"93_Tue Mar 12 2019 11:22:33 GMT+0000 (Coordinated Universal Time)","2019-11-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Main Engine Lubricators for all the units leaking. ","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","O rings of Main Engine lubricator indicators renewed.","2020-03-31T23:59:35","","Completed","2020-02-20T23:59:35","No","No","No","Internal"]
[null,null,null,7658,null,"93_Tue Mar 12 2019 11:25:17 GMT+0000 (Coordinated Universal Time)","2019-11-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","No.02 HFO (P) bunker tank is not used for bunkering atleast in the last 11 months. ","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","No.2 HFO (P) bunker tank cleaned at DD and put in use","2020-03-31T23:59:35","","Completed","2020-02-22T23:59:35","No","No","No","Internal"]
[null,null,null,7659,null,"93_Tue Mar 12 2019 11:27:16 GMT+0000 (Coordinated Universal Time)","2019-11-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","10 nos. mooring ropes put in use since 2014 / 2015 & are already 05 years old & in moderate condition.  ","Deck - Mooring Machinery","Mooring","Equipment Related","","","","","8 mooring ropes received in dry dock put in use and old wasted and damged mooring ropes removed and kept separately marked as condemned ropes.","2020-03-31T23:59:35","","Completed","2020-04-20T23:59:35","No","No","No","Internal"]
[null,null,null,7660,null,"93_Tue Mar 12 2019 11:32:11 GMT+0000 (Coordinated Universal Time)","2019-11-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","All roller fairleads have no record of overhauling & all are not rotating easily. ","Deck - Mooring Machinery","Mooring","Equipment Related","","","","","All roller fairleads overhauled in DD. Bushes and shaft renewed for 18 pieces of fair leads.","2020-03-31T23:59:35","","Completed","2020-04-08T23:59:35","No","No","No","Internal"]
[null,null,null,7661,null,"93_Tue Mar 12 2019 11:35:12 GMT+0000 (Coordinated Universal Time)","2019-11-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","All hatch cover cleats have no record of last overhauling.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","overhauling completed for all the hatches","2020-07-30T23:59:35","","Completed","2020-07-17T23:59:35","No","No","No","Internal","This job has been completed in DD by shipstaff, kindly update it."]
[null,null,null,8957,null,"93_Tue Mar 12 2019 11:13:15 GMT+0000 (Coordinated Universal Time)","2019-11-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","WMFF system in alarm condition/panel abnormal alarm. ","Critical Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","All the flame sensors and the smoke sensors of WMFF system checked, the faulty smoke sensors renewed with new sensors.The panel is normal without any alarms ","2020-01-31T23:59:35","","Completed","2019-12-08T23:59:35","No","No","No","Internal"]
[null,null,null,8958,null,"93_Tue Dec 03 2019 11:35:12 GMT+0000 (Coordinated Universal Time)","2019-11-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","All hatch cover cleats have no record of last overhauling.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","Duplication of previous job.","2020-08-31T23:59:35","","Completed","2020-06-05T23:59:35","No","No","No","Internal","This job is recorded twice, kindly keep only one job in report."]
[null,null,null,7662,null,"93_Fri Apr 12 2019 00:05:32 GMT+0000 (Coordinated Universal Time)","2019-11-22T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Stbd anchor, one fluke shows a bend & anchor not used since last 08 months by the previous management","Deck - Mooring Machinery","Mooring","Equipment Related","","","","","Dye test of anchors carried out and found satisfactory.Owners and Class surveyor are satisfied with the Anchor and hence the job is cancelled.","2020-01-31T23:59:35","","Completed","2020-01-19T23:59:35","Yes","No","No","Internal"]
[null,null,null,7663,null,"93_Wed Dec 04 2019 00:09:37 GMT+0000 (Coordinated Universal Time)","2019-11-22T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Gangway Starboard side ladderstep guard is broken at various places .\t","Miscellaneous","Structural Condn. / WT integrity ","Equipment Related","","","","","Gangway step guard repaired by Shipyard.","2020-03-31T23:59:35","","Completed","2020-04-06T23:59:35","Yes","No","No","Internal"]
[null,null,null,7664,null,"93_Fri Apr 12 2019 00:13:38 GMT+0000 (Coordinated Universal Time)","2019-11-22T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Gangway Stanchions are corroded and wasted.\t","Miscellaneous","Structural Condn. / WT integrity ","Equipment Related","","","","","Gangway stanchions repaired.","2020-03-31T23:59:35","","Completed","2020-05-13T23:59:35","No","No","No","Internal"]
[null,null,null,7665,null,"93_Wed Dec 04 2019 00:18:34 GMT+0000 (Coordinated Universal Time)","2019-11-22T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Cargo hold bilge sounding pipe of cargo hold No.3 Port side, No.4 stbd side and No.9 Port side are broken and sounding the Bilges are not possible.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","","","","","Cargo Hold Bilges sounding pipes renewed in Dry dock after hydroblasting and painted 2 coats epoxy.","2020-03-31T23:59:35","","Completed","2020-04-10T23:59:35","Yes","No","No","Internal"]
[null,null,null,7666,null,"93_Wed Dec 04 2019 02:15:30 GMT+0000 (Coordinated Universal Time)","2019-12-04T23:59:35","Defect","Ship Staff","Ship Staff Insp.","The control block and reduction gear of the Bunker Davit Port side are damaged & missing. The davits were not in use for a long time by previous crew.","Miscellaneous","MARPOL Related","Equipment Related","","","","","Control Block changed,Motor overhauled and davit tried out.Davit is workinng but sluggish as found master valve leaking. Hook and drum and wires de-rusting done. RO for leaking master valve and other required parts raised.","2020-12-15T23:59:35","MOJO200037 - RCVD, MOJO200247- PENDING","Completed","2020-12-01T23:59:35","Yes","No","No","Internal","PO will be supplied at next convenient port"]
[null,null,null,7667,null,"93_15/12/2019 10:53:13 AM","2019-12-08T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","Boiler not firing in auto as well as in manual mode.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","On inspection, the heater found choked, the heater cleaned and fitted back. The boiler tried out and is found working in both auto and manual mode.","2019-12-26T23:59:35","MOJO 190039","Completed","2020-12-26T23:59:35","No","No","No","Internal"]
[null,null,null,7668,null,"93_15/12/2019 10:59:20 AM","2019-12-11T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","The motor of the primary blower of the incinerator showing zero insulation, the blower impeller and the coupling damaged","Miscellaneous","MARPOL Related","Equipment Related","","","","","The primary blower, impeller and the coupling renewed with new spares , tried out working satisfactory. ","2020-03-31T23:59:35","MOJO 190037","Completed","2020-03-25T23:59:35","No","No","No","Internal"]
[null,null,null,24608,null,"93_15 Feb 2022 1:12:57 AM","2020-01-25T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Aft Hyd power pack, Hyd oil cooler S.W outlet pipe passing via generator plateform has several pinholes and showing water leakge.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","The affected two pipe section removed and replaced with new fabricated pipes. Line tested and no further leakge observed.","2020-04-24T23:59:35","","Completed","2022-02-07T23:59:35","No","No","No","Internal"]
[null,null,null,10316,null,"93_30/1/2020 8:00:25 PM","2020-01-27T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","Diesel Generator No.1 ACB linkage found broken and unable to take DG#1  on load","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","ACB renewed with new spare ACB, tried out , working satisfactory","2020-03-31T23:59:35","MOJO200052 ","Completed","2020-03-05T23:59:35","No","No","No","Internal"]
[null,null,null,10317,null,"93_31/1/2020 9:05:26 AM","2020-01-27T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Upper stool space access hatch W/T lid rubber packing channel fully corroded & wasted.","Hull & Tanks","Structural Condn. / WT integrity ","Equipment Related","","","","","Upper stool space access hatch W/T lid rubber packing channel de-rusted, built up with flat bars & rubber packing renewed. ","2020-03-31T23:59:35","","Completed","2020-03-08T23:59:35","Yes","No","No","Internal"]
[null,null,null,12138,null,"93_17/5/2020 11:32:40 AM","2020-05-03T23:59:35","Defect","Ship Staff","Ship Staff Insp.","All hatch cover stoppers are rusted and siezed. Stoppers to be made free.","Cargo Mach.","Cargo / Ballast Systems","External Factors","","","","","Hatch cover stoppers  made free and lubrication carried out.","2020-05-31T23:59:35","","Completed","2020-05-13T23:59:35","No","No","No","Internal"]
[null,null,null,12836,null,"93_30/6/2020 12:25:49 PM","2020-05-04T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Main Engine Unit # 4 FWD – Bearing sensor is defective and upon investigation found sensor wire broken from sensor end. ","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Vessel received the spare in Singapore on 27.08.2020 and sensor renewed with spare received and working fine.","2020-09-15T23:59:35","MOJO200142","Completed","2020-10-01T23:59:35","No","No","No","Internal","Spares will be supplied at next convenient port."]
[null,null,null,12139,null,"93_17/5/2020 11:44:57 AM","2020-05-04T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Garbage drums are leaking and need to be replaced.","Miscellaneous","General Appearance","External Factors","","","","","Leaking garbage drums replaced with new ones.","2020-05-30T23:59:35","","Completed","2020-05-16T23:59:35","No","No","No","Internal"]
[null,null,null,12134,null,"93_17/5/2020 11:37:28 AM","2020-05-10T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Galley Dish washers,  inoperational and need to be replaced.","Miscellaneous","MLC Related","Equipment Related","","","","","NOT REQUIRED","2020-08-30T23:59:35","MOJO200127","Completed","2020-07-16T23:59:35","No","No","No","Internal","PO will be supplied at next convenient port as correct voltage/frequency as per vessel requirement was not available during vessel India call."]
[null,null,null,12135,null,"93_17/5/2020 12:04:08 PM","2020-05-10T23:59:35","Defect","Ship Staff","Ship Staff Insp.","All Accommodation Natural vents hinges are rusted and seized.","Accommodation","Structural Condn. / WT integrity ","External Factors","","","","","All Accommodation Natural vent hinges  De-rusted and made free.","2020-08-20T23:59:35","","Completed","2020-07-29T23:59:35","No","No","No","Internal","Update office work progress on natural vent via weekly maintenance report."]
[null,null,null,12136,null,"93_17/5/2020 11:55:16 AM","2020-05-10T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Elevator shaft access & Maintenance top hatch packing channel is badly De-rusted.","Accommodation","Structural Condn. / WT integrity ","Equipment Related","","","","","Elevator shaft access & Maintenance top hatch packing channel  builtup and packing  changed.","2020-06-05T23:59:35","","Completed","2020-06-05T23:59:35","No","No","No","Internal","Kindly update work progress through weekly maintenance reports."]
[null,null,null,12137,null,"93_17/5/2020 12:08:41 PM","2020-05-10T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Engine room skylight supports are wasted and corroded","Miscellaneous","Structural Condn. / WT integrity ","External Factors","","","","","derusting painting carried out","2020-07-30T23:59:35","","Completed","2020-07-11T23:59:35","No","No","No","Internal"]
[null,null,null,12838,null,"93_30/6/2020 10:31:43 PM","2020-05-14T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Galley Hot plate not working - 2 & 4.","Accommodation","Eng. / Strg. Comp.","Equipment Related","","","","","New hot plate installed in galley, as the system was running on 2 phaase same modified according to manual on 3 phase power supply all are functional.","2020-09-14T23:59:35","MOJO200120","Completed","2020-09-04T23:59:35","No","No","No","Internal","Ro will be supplied by NGM at next convenient port."]
[null,null,null,15134,null,"93_15/8/2020 10:29:44 AM","2020-06-09T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Stern Tube seals - In ballast passage observed oil water emulsion from AFT seal drain and in loaded passage found slight oil leakage into the engine room from the FWD seal.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","System is in under observation for no abnormal water ingress or oil leaks into the engine room. Maker is in the correspondence regarding the same.The leak is minimal and within limits.","2020-12-31T23:59:35","","Completed","2020-12-15T23:59:35","No","No","No","Internal","As per makers slight leakage is allowed."]
[null,null,null,15135,null,"93_15/8/2020 10:38:19 AM","2020-06-09T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Composite Boiler - Unable to fire on VLSFO","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","Vessel is unable to\n\nfire boiler on VLSFO from time of docking due to fouling of the furnace\n\nuptake and the high uptake temperature when VLSFO is used as fuel but don't\n\nhave any such problem while using LSMGO.The \n\ncomposite boiler was checked  by the technician at the DD to resolve issue of\n\nboiler fouling in the month of March/April.Technician was also unable to provide any solution to it.Problem to be investiagated further.Further, boiler technician attended the vessel in Dandong,china and boiler problem rectified.Boiler firing in VLSFO now.\n\n","2020-09-30T23:59:35","","Completed","2020-11-18T23:59:35","No","No","No","Internal","Technician attendance arranged at Dongdong China once vessel go alongside for discharging."]
[null,null,null,15141,null,"93_15/8/2020 10:18:42 AM","2020-06-09T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Topping Up Air Compressor - not building pressure and out of pressure","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related","","","","","Troubleshooting in progress. Vessel was awaiting spares,same received in Singapore. Compressor overhauled with new piston,piston rings and con rod bearings received. Bumping clearance measured and found within maker recommended limits. Compressor tried out and found satisfactory.","2020-09-15T23:59:35","","Completed","2020-09-27T23:59:35","No","No","No","Internal"]
[null,null,null,12837,null,"93_29/6/2020 10:46:57 PM","2020-06-19T23:59:35","Non Conformity","Ship Staff","Ship Staff Insp.","Stbd side Life boat Magnetic Compass is highly erratic & has no match with the ship’s Magnetic compass","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","replaced with new one","2020-08-25T23:59:35","","Completed","2020-07-04T23:59:35","No","No","No","Internal","Kindly revert how much is difference. Make sure while reporting defect, RO no is also recorded in Sea Graph."]
[null,null,null,12839,null,"93_29/6/2020 10:59:02 PM","2020-06-19T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Bridge Clock back light Not working & cannot see time in night time","Navigation - Others","Navigation","Equipment Related","","","","","upon investigation found different type of clock is installed which doesnt have dimmer function for same Ro raised and spares received in singapore and same fixed. ","2020-07-30T23:59:35","MOJO205059","Completed","2020-08-31T23:59:35","No","No","No","Internal","Kindly investigate root cause of malfunction, raise RO for spares required."]
[null,null,null,12840,null,"93_29/6/2020 11:04:23 PM","2020-06-19T23:59:35","Observation","Ship Staff","Ship Staff Insp.","1 No GMDSS walkie talkie has slight issue with rotary switch","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","New walkie talkie supplied at Gwangyang berth,Korea","2021-01-20T23:59:35","","Completed","2021-01-16T23:59:35","No","No","No","Internal","Kindly elaborate issue & revert if rotory switch can be replaced with normal working walkie talkie."]
[null,null,null,12841,null,"93_30/6/2020 12:22:13 PM","2020-06-20T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Main Engine – Unit # 5 Fuel Pump puncture O-rings are found to be leakin slightly. O-rings to be renewed. ","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Puncture valve o-rings renewed.","2020-07-20T23:59:35","","Completed","2020-07-19T23:59:35","No","No","No","Internal","Vsl to rectify during next scavenge space inspection."]
[null,null,null,12843,null,"93_29/6/2020 10:56:36 PM","2020-06-20T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Auto Pilot Course Alteration knob does not work","Navigation - Others","Navigation","Equipment Related","","","","","repaired","2020-08-31T23:59:35","MOJO205060","Completed","2020-08-27T23:59:35","No","No","No","Internal","Does vessel require knob or any other part, kindly investigate & revert."]
[null,null,null,12842,null,"93_29/6/2020 10:53:06 PM","2020-06-22T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Fire line drain valves seized","LSA / FFA","Safety / LSA / FFA","External Factors","","","","","overhauled","2020-07-10T23:59:35","","Completed","2020-07-07T23:59:35","No","No","No","Internal"]
[null,null,null,12847,null,"93_30/6/2020 12:44:17 PM","2020-06-22T23:59:35","Defect","Ship Staff","Ship Staff Insp.","AE 3 - Unit #1 - Fuel Pump delivery valve assembly was found cracked and oil leaking from the seating face of the delivery valve. ","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","AE was immediately stopped and delivery valve assembly replaced by old genuine spare. ","2020-06-22T23:59:35","","Completed","2020-06-22T23:59:35","No","No","No","Internal"]
[null,null,null,12844,null,"93_29/6/2020 10:36:49 PM","2020-06-23T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Hold no. 3 main water ingress alarm not working ","Miscellaneous","Cargo / Ballast Systems","Equipment Related","","","","","Sensor changed with spare received and working satisfactory.","2020-09-30T23:59:35","MOJO190013","Completed","2020-09-28T23:59:35","No","No","No","Internal","NGM will supply at next convenient port."]
[null,null,null,12848,null,"93_29/6/2020 10:50:02 PM","2020-06-23T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Port side embarkation ladder shackles seized ","LSA / FFA","Safety / LSA / FFA","External Factors","","","","","derusting & lubrication done","2020-06-26T23:59:35","","Completed","2020-06-24T23:59:35","No","No","No","Internal"]
[null,null,null,12846,null,"93_29/6/2020 10:40:42 PM","2020-06-24T23:59:35","Non Conformity","Ship Staff","Ship Staff Insp.","Fire line has a hole aft of No. 6 hold","LSA / FFA","Safety / LSA / FFA","External Factors","","","","","leak rectified","2020-07-04T23:59:35","","Completed","2020-07-07T23:59:35","No","No","No","Internal","Revert if fire line can be dismantled & taken to engine workshop for repairs. Confirm vessel has material to renew faulty line as patch work is not acceptable."]
[null,null,null,12845,null,"93_29/6/2020 10:43:40 PM","2020-06-25T23:59:35","Non Conformity","Ship Staff","Ship Staff Insp.","Accomodation block  Fire Hydrants found seized","LSA / FFA","Safety / LSA / FFA","Human Error","","","","","lubrication carried out","2020-07-10T23:59:35","","Completed","2020-07-03T23:59:35","No","No","No","Internal","Kindly rectify defect on earliest as this is safety item. Inform office once valve operation in good condition."]
[null,null,null,12849,null,"93_30/6/2020 12:31:56 PM","2020-06-25T23:59:35","Defect","Ship Staff","Ship Staff Insp.","MAC 1 & 2 - Cooling water inlet magnetic solenoid valve was found always in open condition thereby leading to excessive cooling of compressor as standstill condition.","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related","","","","","Upon investigation , found the timer for magentic solenoid valve operation was defetive and same was replaced with new spare. Compressor test run and found satisfactory.","2020-06-30T23:59:35","","Completed","2020-06-29T23:59:35","No","No","No","Internal"]
[null,null,null,15142,null,"93_17/7/2020 11:45:54 AM","2020-07-03T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Aux. Engine No.3 turning gear limit switch found malfunctioning.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Aux. Engine No.3 turning gear limit switch replaced with the new recieved spare at singapore.","2020-09-15T23:59:35","MOJO200152","Completed","2020-09-14T23:59:35","No","No","No","Internal"]
[null,null,null,15143,null,"93_15/8/2020 10:11:15 AM","2020-07-04T23:59:35","Defect","Ship Staff","Ship Staff Insp.","GE 3 - Voltage Transducer not working and unable to take the generator on load in auto.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Spare received in Singapore on 27.08.2020.Defective voltage transducer replaced with new and found ok. ","2020-08-31T23:59:35","MOJO200151","Completed","2020-08-30T23:59:35","No","No","No","Internal"]
[null,null,null,15144,null,"93_17/7/2020 5:14:41 PM","2020-07-10T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Bilge Pump - not taking suction and efficiency found not optimum.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","","","","","Bilge pump overhauled and found that the stator rubber is damaged. Stator replaced with spare new. Pump tried out. Found normal.","2020-07-15T23:59:35","","Completed","2020-07-12T23:59:35","No","No","No","Internal"]
[null,null,null,15154,null,"93_1/8/2020 8:52:07 AM","2020-07-13T23:59:35","Defect","Ship Staff","Ship Staff Insp.","MAIN AIR COMPRESSOR NO.1 RUNNING COUNTER WAS NOT WORKING.","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related","","","","","MAIN AIR COMPRESSOR NO.1 RUNNING COUNTER REPLACED WITH RECIEVED SPARE.","2020-08-31T23:59:35","MOJO200102","Completed","2020-07-29T23:59:35","No","No","No","Internal"]
[null,null,null,15145,null,"93_17/7/2020 11:48:48 AM","2020-07-14T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Air Compressor was not starting on auto function.\t","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related","","","","","Upon investigation found pressure switch was not operating same rectified and made operational.","2020-07-31T23:59:35","","Completed","2020-07-15T23:59:35","No","No","No","Internal"]
[null,null,null,15146,null,"93_17/7/2020 5:20:37 PM","2020-07-14T23:59:35","Defect","Ship Staff","Ship Staff Insp.","ME FO Flowmeter - found to be erratic and not giving correct reading","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Vessel received the spare new flowmeter in Singapore on 27.08.2020.Old flowmeter was replaced with spare new and flowmeter put in use.","2020-07-31T23:59:35","MOJO200160","Completed","2020-08-29T23:59:35","No","No","No","Internal"]
[null,null,null,15147,null,"93_1/8/2020 9:15:45 AM","2020-07-20T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Provision ref. syatem No.1 suction and discharge pressure gauges found not working. ","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Spare guages recieved in singapore on 27.08.2020.Same renewed.","2020-09-15T23:59:35","MOJO200155","Completed","2020-09-28T23:59:35","No","No","No","Internal"]
[null,null,null,15148,null,"93_1/8/2020 8:48:53 AM","2020-07-21T23:59:35","Defect","Ship Staff","Ship Staff Insp.","ME LO Pump #2 - Auto Standby fucntion not working.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Vessel received the spare in Singapore on 27.08.2020. The defective module replaced with spare new received and pump put on auto standby.","2020-08-31T23:59:35","MOJO200167","Completed","2020-08-28T23:59:35","No","No","No","Internal"]
[null,null,null,15149,null,"93_1/8/2020 9:02:42 AM","2020-07-25T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Fire Bilge & GS pump No.1 found leaking from mechanical seal.\t","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","","","","","Pum dismentaled and overhauled. Renewed mechanical seal and o-rings.","2020-07-31T23:59:35","","Completed","2020-07-30T23:59:35","No","No","No","Internal"]
[null,null,null,15159,null,"93_1/8/2020 6:58:19 PM","2020-07-25T23:59:35","Defect","Ship Staff","Ship Staff Insp.","ME Jacket cooling water pump # 2 - Mechanical seal found leaking.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","","","","","Pump overhauled and mechanical seal changed. ","2020-07-25T23:59:35","","Completed","2020-07-25T23:59:35","No","No","No","Internal"]
[null,null,null,15150,null,"93_28/7/2020 12:39:27 AM","2020-07-26T23:59:35","Observation","Ship Staff","Ship Staff Insp.","X BAND performance,dark pitch black PPI Problem.Radar is very old so CRT Problem.\n\n","Navigation - RADAR","Navigation","Equipment Related","","","","","Technician attanded, problem rectified","2020-08-27T23:59:35","","Completed","2020-08-27T23:59:35","No","No","No","Internal"]
[null,null,null,15151,null,"93_28/7/2020 12:34:45 AM","2020-07-26T23:59:35","Defect","Ship Staff","Ship Staff Insp.","S BAND needs screen change, Targets have started painting on 12NM,and on higher ranges also. Location of Radar is unsuitable/unsafe for night navigation as radar is in chart room\n\n","Navigation - RADAR","Navigation","Equipment Related","","","","","Technician attended , problem rectified","2020-08-30T23:59:35","","Completed","2020-08-27T23:59:35","No","No","No","Internal"]
[null,null,null,15138,null,"93_3/8/2020 11:16:10 PM","2020-08-03T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","HATCH COVERS GUIDE WHEELS ARE RUSTY, NEED TO BE MAINTAINED","Miscellaneous","General Appearance","External Factors","","","","","Hatch cover wheels de-rusted and painted two coats primer and finish yellow highlights.","2021-07-31T23:59:35","","Completed","2021-04-01T23:59:35","No","No","No","Internal","This observation is now more than 7 months old. Pls cancel this & re-raise if still need to be done as max time allowed for any observation to close is 3 months."]
[null,null,null,15139,null,"93_3/8/2020 11:31:04 PM","2020-08-03T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","IN BALLAST CONTROL RM, BALLAST AND DRAFT GAUGES ARE INOPERATIONAL.","Miscellaneous","Cargo / Ballast Systems","Equipment Related","","","","","Air Lines and copper pipes leading to and from the tank to be checked by the service technician in the next dry dock. Same defect was raised in the last dry dock but the attending service technicians from Greece were unable to fix the defect. The defect is captured in Refman.","2025-04-20T23:59:35","","Completed","2021-04-19T23:59:35","Yes","No","No","Internal","This observation is now more than 7 months old. Pls cancel this & re-raise if still need to be done as max time allowed for any observation to close is 3 months."]
[null,null,null,15152,null,"93_3/8/2020 10:54:29 PM","2020-08-03T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","SOME PIPES’ SUPPORTS AND UBOLTS NEED TO BE REPLACED.","Deck - Pipe / Fittings","General Appearance","External Factors","","","","","Renewed ","2020-08-30T23:59:35","","Completed","2020-08-13T23:59:35","No","No","No","Internal"]
[null,null,null,15153,null,"93_3/8/2020 11:20:47 PM","2020-08-03T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","JACKS’ T-PIECES IWO HCs 3/6/8 FOUND WITH BIG CLEARANCE AND MISALIGNED WITH TRACKWAY CAUSING WHEELS TO FALL ASIDE  ","Deck - Machinery","Cargo / Ballast Systems","External Factors","","","","","clearance reduced by bulting up the plate","2020-08-30T23:59:35","","Completed","2020-08-22T23:59:35","No","No","No","Internal"]
[null,null,null,15155,null,"93_3/8/2020 11:26:48 PM","2020-08-03T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","NOTED FEW TRACES OF RECENT LEAKS FM FITTINGS OF BRANCH HYD. PIPES ON DECK","Deck - Machinery","Cargo / Ballast Systems","Equipment Related","","","","","rectified","2020-08-30T23:59:35","","Completed","2020-09-01T23:59:35","No","No","No","Internal"]
[null,null,null,15156,null,"93_3/8/2020 10:59:05 PM","2020-08-03T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","HATCH COVERS TOP PANELS HAVE EXTENSIVE RUST AND NEED TO BE CHIPPED/PAINTED","Deck - Machinery,Miscellaneous","General Appearance","External Factors","","","","","chipping / painting completed for all hatch covers 1 to 9","2020-11-30T23:59:35","","Completed","2020-11-09T23:59:35","No","No","No","Internal"]
[null,null,null,15157,null,"93_15/8/2020 9:44:33 AM","2020-08-07T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Engine Room Crane - STBD side push button was found not operating.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","Found the wire for STBD movement broken. Wire repaired and crane tried out.Found satisfactory.","2020-08-10T23:59:35","","Completed","2020-08-08T23:59:35","No","No","No","Internal"]
[null,null,null,15158,null,"93_15/8/2020 9:26:41 AM","2020-08-08T23:59:35","Defect","Ship Staff","Ship Staff Insp.","RAI-16 module for DPU11 in DPU Cabinet B for alarm and monitoring system is defective.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","Vessel received the spare in Singapore on 27.08.2020.Defective module replaced with spare new programmed module and group alarms put back to normal.","2020-08-31T23:59:35","MOJO205064","Completed","2020-08-28T23:59:35","No","No","No","Internal"]
[null,null,null,15160,null,"93_15/9/2020 11:45:10 PM","2020-08-08T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Fresh water generator Ejector pump triped while running.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","","","","","Upon investingation found the windings were burnt and new spare motor ordered and received at Singapore on 27.08.2020. Same replaced and ejector pump put in use.","2020-08-30T23:59:35","","Completed","2020-08-29T23:59:35","No","No","No","Internal"]
[null,null,null,15161,null,"93_15/8/2020 9:34:26 AM","2020-08-13T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Ejector pump - found not running and stopped.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","","","","","Vessel received new motor in Singapore on 27.08.2020.Motor changed and ejector pump test run. Found satisfactory and put in use.","2020-08-31T23:59:35","MOJO200198","Completed","2020-08-28T23:59:35","No","No","No","Internal"]
[null,null,null,15162,null,"93_31/8/2020 1:32:27 PM","2020-08-15T23:59:35","Defect","Ship Staff","Ship Staff Insp.","DG 2 - It was observed that DG 2 couldn't take load more than 530 KW.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Suspected problem with the governor linkage and needs adjusted. Maker was consulted and a governor technician was arranged for servicing at Singapore on 27.08.2020. He had adjusted the governor linkage and now the GE 2 can take load upto 630 KW.","2020-08-31T23:59:35","","Completed","2020-08-27T23:59:35","No","No","No","Internal"]
[null,null,null,15163,null,"93_31/8/2020 12:52:36 PM","2020-08-22T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Main Engine #1 and #3 unit fuel pump punture valves were found to be sluggish attimes. ","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Units 1 and 3 punture valves replaced with spare overhauled punture valves.","2020-08-31T23:59:35","","Completed","2020-08-22T23:59:35","No","No","No","Internal"]
[null,null,null,15140,null,"93_15/9/2020 11:37:48 PM","2020-09-04T23:59:35","Defect","Ship Staff","Ship Staff Insp.","The Kongsberg alarm monitoring system ROS1 is inoperational as the CPU doesn't reboot.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","Kongsberg technician attended the vessel at Dandong,China and system has been upgraded sucessfully .","2020-10-05T23:59:35","","Completed","2020-11-19T23:59:35","No","No","No","Internal","Makers arranged at China once vsl go alongside for discharging"]
[null,null,null,15164,null,"93_15/10/2020 12:42:51 PM","2020-10-02T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Oily Water Separator - 3 way valve's 3/2 Directional control valve was found malfunctioning. ","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","3/2 DC valve replaced with spare new and OWS alarm and 3-way valve fuction checked found working satisfactory.","2020-10-02T23:59:35","","Completed","2020-10-02T23:59:35","No","No","No","Internal"]
[null,null,null,15165,null,"93_31/10/2020 4:00:15 AM","2020-10-03T23:59:35","Defect","Ship Staff","Ship Staff Insp.","FO Overflow tank remote sensor not working","Hull & Tanks","Eng. / Strg. Comp.","Equipment Related","","","","","Same rectified with new spare sensor received.","2020-10-31T23:59:35","","Completed","2020-10-23T23:59:35","No","No","No","Internal"]
[null,null,null,15166,null,"93_31/10/2020 9:00:39 AM","2020-10-04T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Main Engine Turning gear found emergency stop switch not working .","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Found wiring damaged for the switch and same rectified. Tried out and found satisfactory.","2020-10-31T23:59:35","","Completed","2020-10-23T23:59:35","No","No","No","Internal"]
[null,null,null,15167,null,"93_15/10/2020 5:04:53 PM","2020-10-05T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Emergency Fire pump priming unit - Linkage was found broken ","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","","","","","The linkage was removed welded and put back and same working now. R.O MOJO200234 raised for priming unit , for using in future. ","2020-10-15T23:59:35","RO MOJO200234","Completed","2020-10-05T23:59:35","No","No","No","Internal"]
[null,null,null,15168,null,"93_31/10/2020 8:42:59 AM","2020-10-18T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Bridge Toilet reported not working","Deck - Machinery,E/R - Aux. Mach.","Crew Management","Equipment Related","","","","","Toilet removed from the base and membrane valve renewed. Toilet tried out and found satisfactory.","2020-10-31T23:59:35","","Completed","2020-10-30T23:59:35","No","No","No","Internal"]
[null,null,null,15169,null,"93_16/11/2020 8:52:57 AM","2020-11-10T23:59:35","Defect","Ship Staff","Ship Staff Insp.","GE 1 - Scavenge air leak from the blower side of the turbocharger leading to high exhaust temperature of the units","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Found that the gasket on the blower side of turbcharger is damaged and air leaking.Hence the cause for high exhaust temperature in the units.Same attended and gasket renewed.","2020-11-15T23:59:35","","Completed","2020-11-12T23:59:35","No","No","No","Internal"]
[null,null,null,16021,null,"93_23/12/2020 2:46:03 PM","2020-12-23T23:59:35","Observation","Ship Staff","Ship Staff Insp.","WBT flow through valves derusting for no. 5 P/S ","Miscellaneous","General Appearance","External Factors","","","","","Derusting to be done ","2021-01-31T23:59:35","","Completed","2021-01-06T23:59:35","No","No","No","Internal"]
[null,null,null,16022,null,"93_22/12/2020 11:52:53 PM","2020-12-23T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Hatch coamings derusting","Deck - Machinery","General Appearance","Equipment Related","","","","","Derusted / Painted","2021-03-30T23:59:35","","Completed","2021-01-07T23:59:35","No","No","No","Internal"]
[null,null,null,16023,null,"93_23/12/2020 12:04:57 AM","2020-12-23T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Restricting arms derusting no 5","Deck - Machinery","General Appearance","Equipment Related","","","","","Derusted / Painted","2021-01-31T23:59:35","","Completed","2021-01-08T23:59:35","No","No","No","Internal"]
[null,null,null,16024,null,"93_23/12/2020 5:08:50 PM","2020-12-23T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Slight steam leak above cascade tank to arrest and rectify.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Steam leakage rectified","2021-01-15T23:59:35","","Completed","2020-12-28T23:59:35","No","No","No","Internal"]
[null,null,null,16025,null,"93_23/12/2020 5:18:00 PM","2020-12-23T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Differential pressure switch not working.Upon investigation found the switch defective.Same in order and needs to be replaced when recieved. ","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Defective differential pressure replaced","2021-01-15T23:59:35","MOJO200250","Completed","2021-03-20T23:59:35","No","No","No","Internal"]
[null,null,null,16026,null,"93_23/12/2020 5:24:07 PM","2020-12-23T23:59:35","Observation","Ship Staff","Ship Staff Insp.","E/R 2nd Deck- Local signal mast column alarm rotatory lamp not working. To be investigated and rectified.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","Local signal mast column alarm rotatory lamp was found to be defective and same replaced.","2021-01-15T23:59:35","","Completed","2020-12-27T23:59:35","No","No","No","Internal"]
[null,null,null,16027,null,"93_23/12/2020 5:29:06 PM","2020-12-23T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Fresh water Generator Dosing tank leakage to rectify and the hose to be renewed.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Found the hose couplings loose and leaking from the sealing O-rings. Same rectified.","2021-01-15T23:59:35","","Completed","2021-01-03T23:59:35","No","No","No","Internal"]
[null,null,null,16028,null,"93_23/12/2020 5:33:48 PM","2020-12-23T23:59:35","Observation","Ship Staff","Ship Staff Insp.","E/R- Bottom platform Air leakage from service air valve to arrest and rectify","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Air leakage from service air valve arrested and rectified.Found air leaking from the sealing flanges. Same rectified.","2021-01-15T23:59:35","","Completed","2020-12-30T23:59:35","No","No","No","Internal"]
[null,null,null,16029,null,"93_23/12/2020 5:38:44 PM","2020-12-23T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Leakage on M.E F.O Auto filter to rectifyand leaking top o-ring to change.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","M.E Auto filter leakage rectified","2021-01-15T23:59:35","","Completed","2020-12-25T23:59:35","No","No","No","Internal"]
[null,null,null,16030,null,"93_23/12/2020 5:44:43 PM","2020-12-23T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Cosmetic condition of the trunking in 2nd platform STBD side to improve.To be cleaned and painted.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Trunking in STBD side 2nd platform cleaned and paint.","2021-01-15T23:59:35","","Completed","2021-01-01T23:59:35","No","No","No","Internal"]
[null,null,null,16031,null,"93_23/12/2020 5:56:51 PM","2020-12-23T23:59:35","Observation","Ship Staff","Ship Staff Insp.","No.1 Fuel oil supply pump Mechanical seal leakage to rectify.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","","","","","No.1 Fuel oil supply pump mechanical seal  changed.","2021-01-15T23:59:35","","Completed","2020-12-24T23:59:35","No","No","No","Internal"]
[null,null,null,16032,null,"93_23/12/2020 6:00:04 PM","2020-12-23T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Main Breaker switch is found broken, breaker switch to replace.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","Main Breaker switch replace with spare.","2021-01-15T23:59:35","","Completed","2020-12-28T23:59:35","No","No","No","Internal"]
[null,null,null,16033,null,"93_23/12/2020 6:04:05 PM","2020-12-23T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Duct keel fan is making abnormal noise, same need to be checked and problem attended.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","Duck keel fan removed, damaged foundation repaired and fabricated new and motor overhauled.Installed in place.Tried out found satisfactory.","2021-01-15T23:59:35","","Completed","2021-01-05T23:59:35","No","No","No","Internal"]
[null,null,null,16034,null,"93_23/12/2020 2:15:40 PM","2020-12-23T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Restricting arms derusting no. 6","Deck - Machinery","General Appearance","Equipment Related","","","","","Derusted / Painted","2021-01-31T23:59:35","","Completed","2021-01-08T23:59:35","No","No","No","Internal"]
[null,null,null,16035,null,"93_23/12/2020 2:17:44 PM","2020-12-23T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Restricting arms derusting no. 7","Deck - Machinery","General Appearance","Equipment Related","","","","","Derusted / Painted","2021-01-31T23:59:35","","Completed","2021-01-08T23:59:35","No","No","No","Internal"]
[null,null,null,16036,null,"93_23/12/2020 2:19:39 PM","2020-12-23T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Restricting arms derusting no. 8","Deck - Machinery","General Appearance","Equipment Related","","","","","Derusted / Painted","2021-01-31T23:59:35","","Completed","2021-01-08T23:59:35","No","No","No","Internal"]
[null,null,null,16037,null,"93_23/12/2020 2:38:19 PM","2020-12-23T23:59:35","Observation","Ship Staff","Suptd. Insp.","WBT flow through valves derusting for no. 3 P/S","Miscellaneous","General Appearance","External Factors","","","","","Derusted / Painted","2021-01-31T23:59:35","","Completed","2021-01-06T23:59:35","No","No","No","Internal"]
[null,null,null,16038,null,"93_23/12/2020 2:21:08 PM","2020-12-23T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Restricting arms derusting no. 9","Deck - Machinery","General Appearance","Equipment Related","","","","","Derusted / Painted","2021-01-31T23:59:35","","Completed","2021-01-08T23:59:35","No","No","No","Internal"]
[null,null,null,16039,null,"93_23/12/2020 5:52:36 PM","2020-12-23T23:59:35","Observation","Ship Staff","Ship Staff Insp.","No.1 Hot plate found not working, to be replaced with spare recieved.","Elect. Mach. & Equip.","Crew Management","Equipment Related","","","","","Hot plate replaced with spare and made operational.","2021-01-15T23:59:35","","Completed","2020-12-30T23:59:35","No","No","No","Internal"]
[null,null,null,16040,null,"93_23/12/2020 2:43:39 PM","2020-12-23T23:59:35","Observation","Ship Staff","Ship Staff Insp.","WBT flow through valves derusting for no. 4 P/S ","Miscellaneous","General Appearance","External Factors","","","","","Derusted / Painted","2021-01-31T23:59:35","","Completed","2021-01-06T23:59:35","No","No","No","Internal"]
[null,null,null,16894,null,"93_6/1/2021 10:24:29 AM","2021-01-05T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Vaccum Sewage System - No: 1 Vaccum pump was tripping on overload. Pump & motor removed and both overhauled and tried out still found the overload trip activating. Checked the electrical system found , moulded case CB ( TYPE- GV2-ME10 + GV2-AE11) malfunctioning","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","","","","","Pump & motor removed and both overhauled and tried out still found the overload trip activating. Checked the electrical system found , moulded case CB ( TYPE- GV2-ME10 + GV2-AE11) malfunctioning.vessel is currently running the No: 1 Vaccum pump (as it was overhauled) by using the No: 2 moulded circuit breaker of No:2 pump’s circuit. NO:1 moulded CB is defective for which we have raised RO - MOJO210011(Item no:4). Same  changed .","2021-04-10T23:59:35","MOJO210011","Completed","2021-04-16T23:59:35","No","No","No","Internal","This has been supplied to vessel in Korea on 16th Mar'21, kindly check & revert reason for not closing it."]
[null,null,null,18568,null,"93_14/02/2021 04:54:35","2021-01-21T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Water Seepage from No.6 Cargo Hold (Heavy weather Ballast hold) to No.4 WBT Port side.","Hull & Tanks","Structural Condn. / WT integrity ","External Factors","","","","","Repaired the leak from the welding seam in the mid trunk connecting TST with Double Bottom inside No.4 WBT Port side. ","2021-02-05T23:59:35","","Completed","2021-02-03T23:59:35","No","No","No","Internal"]
[null,null,null,18569,null,"93_14/02/2021 04:58:32","2021-01-25T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Water leaking from Level Gauge Pipe of No.5 WBT Port side into No.9 Cargo hold.","Hull & Tanks","Structural Condn. / WT integrity ","External Factors","","","","","The section of Level gauge pipe from the tank top to 1 meter high renewed with new one. ","2021-02-05T23:59:35","","Completed","2021-02-04T23:59:35","No","No","No","Internal"]
[null,null,null,18570,null,"93_13/02/2021 12:33:45","2021-01-27T23:59:35","Critical Equipment","Ship Staff","Ship Staff Insp.","During the Chief Engineer's rounds, it was observed that the Pilot Bottle Cabinet of CO2 releasing mechanism was broken and shattered to pieces.","LSA / FFA","Emgcy. Systems","Behaviour Based","","","","","Cabinet of the Pilot bottles to release CO2 was repaired and fitted back.","2021-02-01T23:59:35","","Completed","2021-02-02T23:59:35","No","No","No","Internal"]
[null,null,null,18571,null,"93_14/02/2021 05:04:29","2021-02-08T23:59:35","Critical Equipment","Ship Staff","Ship Staff Insp.","Hatch Cover Pumps unable to build sufficient continuous pressure for hatch operation.","Cargo Mach.","Cargo / Ballast Systems","Behaviour Based","","","","","Hatch Cover pumps serviced ashore & fitted back , pressure setting done .Complete system oil change carried out . 2  pumps recieved & kept as spare ","2021-02-15T23:59:35","","Completed","2021-02-13T23:59:35","No","No","No","Internal"]
[null,null,null,18553,null,"93_14/02/2021 05:07:26","2021-02-11T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Oil Leaking from side from the control Lever Block of Mooring Winch / Windlass Port and Stbd.","Deck - Mooring Machinery","Mooring","Equipment Related","","","","","Blocks checked , leak rectified ","2021-04-15T23:59:35","","Completed","2021-04-08T23:59:35","No","No","No","Internal"]
[null,null,null,18554,null,"93_14/02/2021 08:05:12","2021-02-12T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Seepage from No.4 WBT Stbd into No.6 Cargo Hold.","Hull & Tanks","Structural Condn. / WT integrity ","External Factors","","","","","The leak was arrested and the crack was grinded, v gauged, and was filled with rounds of welding. Also extra rod welded in the tank side.","2021-05-01T23:59:35","","Completed","2021-04-13T23:59:35","No","No","No","Internal"]
[null,null,null,18572,null,"93_16/2/2021 10:40:56 AM","2021-02-14T23:59:35","Defect","Ship Staff","Ship Staff Insp.","2 vertical ladders in the Funnel area found to be having crack at the bottom weld seam","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","The ladders have been fixed properly now with nut & bolts arrangement . Checked all the ladders in the funnel as a precautionary measure  ","2021-03-08T23:59:35","","Completed","2021-03-08T23:59:35","No","No","No","Internal"]
[null,null,null,18573,null,"93_14/02/2021 08:08:00","2021-02-14T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Fair Lead Roller found cracked on Poop Deck Port side.","Deck - Pipe / Fittings","Mooring","External Factors","","","","","Fair lead roller was supplied at yeoungheung and replaced the damaged one.","2021-04-01T23:59:35","MOJO215011 / MOJO210040","Completed","2021-03-17T23:59:35","No","No","No","Internal"]
[null,null,null,18574,null,"93_07/03/2021 13:57:32","2021-02-28T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Few Watertight doors found not sealing completelly.","Accommodation","Structural Condn. / WT integrity ","Equipment Related","","","","","Watretight door packing  renewed and packing channel completely de-rusted. Dogs and levers  greased and tightened as required. Wasted Packing channel repaired as required.","2021-03-12T23:59:35","","Completed","2021-03-12T23:59:35","No","No","No","Internal"]
[null,null,null,18575,null,"93_07/03/2021 14:03:48","2021-03-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Starboard side entry watertight door retaining channel packing lip found to be wasted at few locations and need to be cropped and renewed.","Accommodation","Structural Condn. / WT integrity ","External Factors","","","","","Watertight door retaining channel packing lip  cropped and renewed.","2021-03-12T23:59:35","","Completed","2021-03-12T23:59:35","No","No","No","Internal"]
[null,null,null,18576,null,"93_07/03/2021 14:46:30","2021-03-02T23:59:35","Defect","Ship Staff","Mooring Audit","During Mooring Audit it was found that Mooring hawsers of different type and lay were rigged on the forward spring and head line. Also one of the head ropes were found damaged. The vessel has no new spare ropes.","Deck - Mooring Machinery","Mooring","Inappropriate Procedure","","","","","The ropes have been interchanged with the 2 Nylon ones on the spring and all polypropylene on the Head, stern and aft springs. The damaged Head rope was replaced with one new spare rope. Requisition for the  New spare ropes has been raised and same is awaited for supply. been ","2021-06-30T23:59:35","MOJO210067","Completed","2021-03-16T23:59:35","No","No","No","Internal"]
[null,null,null,18580,null,"93_07/03/2021 14:16:26","2021-03-02T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Stopper arm of all hatch covers found siezed and inoperational.","Cargo Mach.","Cargo / Ballast Systems","External Factors","","","","","Stopper arm of all hatc chovers  made frree, lubricated and  moved once every week during long voyages.","2021-03-12T23:59:35","","Completed","2021-03-04T23:59:35","No","No","No","Internal"]
[null,null,null,18552,null,"93_07/03/2021 14:49:45","2021-03-05T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Doors at entrance of accommodation on Port and stbd side found not to be closing completely and the frame is completely wasted and rusted.","Accommodation","General Appearance","Inappropriate Procedure","","","","","The frame of the doors repaired. Latch replaced. Door closing completely.","2021-06-15T23:59:35","MOJO210089","Completed","2021-06-05T23:59:35","No","No","No","Internal","This observation is overdue, pls let us know vessel intention to close it."]
[null,null,null,18555,null,"93_8/3/2021 3:03:09 PM","2021-03-06T23:59:35","Observation","Ship Staff","Engineering Audit","Reference to safety flash No.109 ( oil leak in purifier room ) , it was noticed that vessel does not have the original type O rings for the various pump filters & also for the Backwash filters , same are important to avoid any oil spills","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related,Inappropriate Procedure","","","","","Inventory taken , O rings for Backwash filter arranged in boxes","2021-04-25T23:59:35","","Completed","2021-04-20T23:59:35","No","No","No","Internal","Observation is not valid till equipment has some problem. Kindly remove it & order O-Rings as required."]
[null,null,null,18577,null,"93_8/3/2021 2:53:28 PM","2021-03-06T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Drinking water tank Gauge glass union has leak . This tank was not in use for long time . Recently the tank cleaned & put in use . After putting in use , this leak was noticed ","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Water now filled in Drinking water tank . Gauge glass connection repaired ","2021-03-10T23:59:35","","Completed","2021-03-28T23:59:35","No","No","No","Internal"]
[null,null,null,18578,null,"93_8/3/2021 3:22:56 PM","2021-03-06T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","Noticed that Forward electric whistle was not working . Upon investigation found the motor insulation 0 , terminal box damaged with water inside & bolts missing for the terminal box cover causing it to remain open  without any weaher protection ","Critical Equip.","Navigation","Equipment Related,External Factors,Human Error,Inappropriate Procedure","","","","","Requisition MOJO210033 raised , same acknowledged by office & spares recieved as per  as per Requisition MOJO215008.Installed , now working ","2021-03-15T23:59:35","","Completed","2021-03-17T23:59:35","No","No","No","Internal"]
[null,null,null,18556,null,"93_8/3/2021 2:36:02 PM","2021-03-07T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","It has been  checked confirmed that both the Laundry Heaters are not working & in damaged  condition  , the main part / the coil is burnt & other relevant parts like thermostat etc damaged  , whole heater in bad rusted condition \n\nCrew Laundry : The heating element ‘ Coil ‘ not heating up , whole heater in bad rusted condition , was cleaned / tried to rectify but since the coil is not working so cannot do much there","Elect. Mach. & Equip.","MLC Related","Equipment Related","","","","","Wrong supply Heaters  landed at Korea, upon receival same will be fitted in place","2021-08-30T23:59:35","MOJO215017","Completed","2021-09-10T23:59:35","No","No","No","Internal","Vsl to be touch with procure for supply of correct parts."]
[null,null,null,18579,null,"93_8/3/2021 2:44:49 PM","2021-03-07T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Both Laundry Dryers defective . Noticed the Officers laundry Dryer belt broken , temporary made operational by fixing a Nylon strap in between sewed along with Loctite . Also the Heater inside the Dryer was repaired by fixing / renewing  the connections , cleaning the whole system . It is temporarily working but cannot say how long it will last (  was not in use for a very long time )\n\nPlease note : This is the only Dryer in Officers laundry ( for both Boiler suits & General clothes ) which also working temporarily with above modifications \n\nCrew Laundry Dryer  : Drum is rusted completely for the dryer , Belt is broken & Dryer s Heater insulation is 0 (  was not in use for a very long time ) \n\n","Elect. Mach. & Equip.","MLC Related","Equipment Related","","","","","Requisition MOJO210069 made , Dryers recieved ,  ","2021-03-15T23:59:35","","Completed","2021-03-20T23:59:35","No","No","No","Internal"]
[null,null,null,18557,null,"93_8/3/2021 3:34:48 PM","2021-03-08T23:59:35","Defect","Ship Staff","Ship Staff Insp.","AE Supply Pump No.1 was leaking badly from the mechanical seal . Pump overhauled , leak stopped , however the pressure of the pump is low , the Gears need to be renewed to achieve proper pressure","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","","","","","Spares recieved , Pump overhaued , now ok ","2021-04-30T23:59:35","MOJO210048","Completed","2021-05-24T23:59:35","No","No","No","Internal"]
[null,null,null,18558,null,"93_8/3/2021 5:05:47 PM","2021-03-08T23:59:35","Defect,Observation","Ship Staff","Ship Staff Insp.","The whole cable from the crane side up to the remote is in damaged condition causing the remote to sometimes ‘ not operate ‘ the crane  , Also the condition of wires inside the push button box  is not good \n\nThis  special 15 core ( VCT-15 c ) cable along with the remote push button box needs to be changed","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related,External Factors","","","","","Requisition MOJO210041 ( ER crane Remote push button switch & cable ) recieved , now ok ","2021-06-20T23:59:35","MOJO210041","Completed","2021-07-05T23:59:35","No","No","No","Internal","Spares ready in Korea & will be supplied to after during discharge call in May'21."]
[null,null,null,18559,null,"93_8/3/2021 5:13:23 PM","2021-03-08T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Observed that the Sluice door operation of the Incineator is erratic / defective . This is because of the faulty pneumatic Direction control valve ( 3 by 2 valve ) , tried to clean / overhaul the same but still the same problem is there . Also noticed taht the electrode unit of the primary burner & its hawse pipe condition is not good","Critical Equip.,E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Changed the 3/2 valve with new spare , now ok ","2021-04-30T23:59:35","MOJO210099","Completed","2021-06-02T23:59:35","No","No","No","Internal","Vessel to raise new RO as MOJO210042 is already closed & forward to all concerned in order to supply in time."]
[null,null,null,18560,null,"93_8/3/2021 5:42:18 PM","2021-03-08T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Galley waste disposer ( Disperator )  found to be not working . It was brought down to workshop & opened up , found the contactor , relay & the unit damaged","Elect. Mach. & Equip.,Miscellaneous","MARPOL Related","Equipment Related","","","","","Requsition MOJO 210059 recently recieved , contactor & replay renewed.","2021-08-20T23:59:35","MOJO 210059 ","Completed","2021-07-10T23:59:35","No","No","No","Internal","Make sure to mention RO no in PO Ref NO in DDRL as same is missing in so many observations. Spares confirmed & will be supplied at next convenient port."]
[null,null,null,18585,null,"93_8/3/2021 5:16:56 PM","2021-03-08T23:59:35","Defect","Ship Staff","Ship Staff Insp.","AE Backwash filter is not in use due to faulty PCB , bypass filter is in use , for safety , every 3 to 4  days this filter is cleaned to always ensure sufficient line fuel pressure ","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Requisition MOJO210031 recieved , fitted in place , now working good so AE Backwash filter working now ","2021-03-15T23:59:35","","Completed","2021-03-20T23:59:35","No","No","No","Internal"]
[null,null,null,18561,null,"93_27/3/2021 9:05:22 PM","2021-03-18T23:59:35","Defect","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","Some Numerals of the forward and aft draft marks were not clearly readable","Hull & Tanks","Cargo / Ballast Systems","External Factors","","","","","Draft Marks will be painted at the next suitable opportunity.","2021-06-01T23:59:35","","Completed","2021-04-10T23:59:35","No","No","No","External"]
[null,null,null,18562,null,"93_27/3/2021 9:18:55 PM","2021-03-18T23:59:35","Defect","Others (Eg. Insurance etc.)","OM Insp. (Eg. SIRE / CDI etc.)","Random checks indicated that the following hatch cover rubbers\n\npermanently deformed / set groove in excess of the recommended tolerance\n\nNo.2 S (Aft) 15.68,  No.3 P (Aft) 14.74 mm , No.4P (Fwd Corner) 15.59 mm\n\nNo.4 S (Fwd) 15.71mm & No.6 P(Aft Corner) 14.02 mm.\n\nRubber packing size 94 x 50mm. Manufacturer's design compression 12mm\n\nand discard criteria 6 mm.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","Rubber packings to be checked and renewed as required at the next available opportunity.","2021-06-01T23:59:35","","Completed","2021-04-10T23:59:35","No","No","No","External"]
[null,null,null,18563,null,"93_27/3/2021 9:47:51 PM","2021-03-18T23:59:35","Observation","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","It is recommended that the same type / material mooring ropes can be used \n\non the same direction / lead. Presently head lines, stern lines and forward\n\nbreast lines were not the same types. There were three types of mooring \n\nprovided onboard. Dia 60, 62 and 64 mm/ 8 strands and 24 strands/\n\nPP & PE mixed and nylon.","Deck - Mooring Machinery","Mooring","External Factors","","","","","Mooring ropes  changed as per recommendation and in consultation with the office. ","2021-06-01T23:59:35","MOJO210084","Completed","2021-04-02T23:59:35","No","No","No","External"]
[null,null,null,18564,null,"93_27/3/2021 10:44:07 PM","2021-03-18T23:59:35","Observation","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","It is recommended that the brake rendering markings (rendering capacity \n\nand tension limit) be clearly marked on the mooring winch spindle","Deck - Mooring Machinery","Mooring","External Factors","","","","","Brake rendering marking clearly marked and a pointer is installed in location permanently after the brake testing. Annual Brake testing done on 19 April 2021","2021-05-01T23:59:35","","Completed","2021-04-19T23:59:35","No","No","No","External"]
[null,null,null,18565,null,"93_27/3/2021 10:53:35 PM","2021-03-18T23:59:35","Defect","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","In cargo Hold #1 - supporting members and guardrails of the upper platform \n\nand lower platform for the Australian ladder were cracked, broken and\n\ndeformed. The Guradrail of the lower platform on the forward vertical \n\nladder was detatched.\n\n","Hull & Tanks","Cargo / Ballast Systems","External Factors","","","","","Repairs on Australian Ladder and Vertical ladder of No.1 Cargo hold carried out and supporting angle bars and welded. Also an extra supporting member welded below the australian ladder. The top and bottom platforms are now straight and welded in position.","2021-04-06T23:59:35","","Completed","2021-04-06T23:59:35","No","No","No","External"]
[null,null,null,18581,null,"93_27/3/2021 9:23:31 PM","2021-03-18T23:59:35","Defect","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","It was noted that there is only one securing point for the ladder for the \n\nforward Liferaft embarkation ( Port and Stbd)","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","Old Pad eye removed and two new pad eyes welded in location for rigging forward embarkation ladder.","2021-04-01T23:59:35","","Completed","2021-03-27T23:59:35","No","No","No","External"]
[null,null,null,18582,null,"93_27/3/2021 10:50:15 PM","2021-03-18T23:59:35","Defect","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","The unsafe practice of using shackles over the side ropes between steps \n\nto secure the pilot ladder was found during the inspection.","Miscellaneous","Safety / LSA / FFA","External Factors","","","","","The use of shackle on pilot ladder is stopped and the all crew briefed about the same. Separate and designated Manila rope used for securing Pilot Ladder.","2021-05-01T23:59:35","","Completed","2021-03-25T23:59:35","No","No","No","External"]
[null,null,null,18583,null,"93_27/3/2021 10:46:13 PM","2021-03-18T23:59:35","Defect","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","Several parts on the strands of the two (2) mooring ropes ( one of the \n\nforward spring and aft spring line) were noticably damaged.","Deck - Mooring Machinery","Mooring","External Factors","","","","","Damaged mooring ropes to be replaced with the new ones.","2021-06-01T23:59:35","","Completed","2021-03-31T23:59:35","No","No","No","External"]
[null,null,null,18584,null,"93_27/3/2021 9:44:37 PM","2021-03-18T23:59:35","Defect","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","Handrail Grips on the roof of the port lifeboat were cracked and detached \n\nSecuring bolts for the grip wre loosening and missing","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","Handrail Grips on the roof of the port lifeboat were repaired and loosening bolts fitted securedly.","2021-04-01T23:59:35","","Completed","2021-03-24T23:59:35","No","No","No","External"]
[null,null,null,18714,null,"93_18/4/2021 6:49:29 AM","2021-03-19T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Pilot ladder step broken while heaving up the ladder. Same to be replaced with a new one.","Miscellaneous","Safety / LSA / FFA","External Factors","","","","","New Piulot ladder received is installed in location and is in use.","2021-05-20T23:59:35","MOJO210082","Completed","2021-05-12T23:59:35","No","No","No","Internal","New ladder will be supplied at next covenient port."]
[null,null,null,18566,null,"93_27/3/2021 10:57:36 PM","2021-03-27T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Sounding pipe of No.7 Cargo hold found broken and detached from location.","Hull & Tanks","Cargo / Ballast Systems","External Factors","","","","","New sndg pipe to be welded in next dry dock. Defect added to Refman for dry dock.","2025-04-01T23:59:35","","Completed","2021-05-01T23:59:35","Yes","No","No","Internal","Pls prepare specs in Refman & forward export file for office review."]
[null,null,null,18725,null,"93_18/4/2021 6:41:11 AM","2021-04-01T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Emergency Generator room Exhaust vent to be thoroughly derusted and the packing to be renewed.","E/R - Aux. Engine","Emgcy. Systems","External Factors","","","","","Emergency Generator room Exhaust vent  thoroughly derusted and the packing  renewed.","2021-04-20T23:59:35","","Completed","2021-04-14T23:59:35","No","No","No","Internal"]
[null,null,null,18713,null,"93_18/4/2021 7:08:11 AM","2021-04-03T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Due to the age of the vessel and regular wear and tear it was observed that the Lifeboat top hatch hinges have been wasted, dogs look worn.","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","To be replaced after receiving spare","2021-07-01T23:59:35","MOJO210092","Completed","2021-09-15T23:59:35","No","No","No","Internal","This observation is now more than 1 year old. Pls cancel this & re-raise if still need to be done as max time allowed for any observation to close is 3 months."]
[null,null,null,15136,null,"93_3/8/2020 10:45:03 PM","2021-04-03T23:59:35","Observation","Ship Staff","Ship Staff Insp.","BUNKER LINE, FIRE LINE, MAIN HYD. LINE, FW LINE, CABLE PIPE AND ASSOCIATED FITTINGS FOUND WITH SPOT RUST","Deck - Pipe / Fittings","General Appearance","External Factors","","","","","derusting / painting in progress.","2021-07-03T23:59:35","","Completed","2021-08-15T23:59:35","No","No","No","Internal","This observation is now more than 1 year old. Pls cancel this & re-raise if still need to be done as max time allowed for any observation to close is 3 months."]
[null,null,null,15137,null,"93_3/8/2020 10:51:45 PM","2021-04-03T23:59:35","Observation","Ship Staff","Ship Staff Insp.","AIR PIPE (SEVERAL AREAS) AND BRANCHES OF HYD. PIPE IWO COAMINGS AND CONTROL STANDS FOUND RUSTY AND NOTED SMALL LEAKS FM FITTINGS","Deck - Pipe / Fittings","General Appearance","External Factors","","","","","Leaks rectified. Derusting & painting planned with hydro blaster.","2021-08-01T23:59:35","","Completed","2021-08-15T23:59:35","No","No","No","Internal","This observation is now more than 7 months old. Pls cancel this & re-raise if still need to be done as max time allowed for any observation to close is 3 months."]
[null,null,null,18715,null,"93_18/4/2021 6:37:39 AM","2021-04-04T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Fire line found to be leaking from two locations on main deck Port side.","Deck - Pipe / Fittings","Emgcy. Systems","External Factors","","","","","Dressor coupling to be renewed and replaced with the new one. The old dressor coupling to be removed, the pipe to be de-rusted and painted and the new one to be installed in location. After repairs the fire line to be tested.","2021-04-20T23:59:35","","Completed","2021-04-20T23:59:35","No","No","No","Internal","Vessel to attend to leakage rectification before calling loading port in Australia."]
[null,null,null,7557,null,"93_Tue Feb 12 2019 09:44:01 GMT+0000 (Coordinated Universal Time)","2021-04-04T23:59:35","Defect","Ship Staff","Ship Staff Insp.","All MS pipe lines on deck including hydraulic lines & electric conduit pipes show heavy corrosion at many places.","Deck - Pipe / Fittings","General Appearance","Equipment Related","","","","","Hydroblasting & painting in progress. ","2021-07-15T23:59:35","","Completed","2021-08-15T23:59:35","Yes","No","No","Internal","This observation is now more than 1.7 year old. Pls cancel this & re-raise if still need to be done as max time allowed for any observation to close is 3 months."]
[null,null,null,18567,null,"93_04/04/2021 13:18:28","2021-04-04T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Port side Gangway Spindle shaft found holed at the support piece area due to corrosion.","Miscellaneous","Cargo / Ballast Systems","External Factors","","","","","The damaged  spindle shaft section renewed.","2021-05-01T23:59:35","","Completed","2021-04-18T23:59:35","No","No","No","Internal","Pls carryout job on earliest as related to gangway."]
[null,null,null,18716,null,"93_18/4/2021 7:01:14 AM","2021-04-05T23:59:35","Defect","Ship Staff","Ship Staff Insp.","It was observed that the Port side lifeboat forward and aft gripes were in a poor condition with the vinyl coating completely damaged exposing the wires.","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","Vessel renewed the forward and aft gripes of port side lifeboat at Kwangyang after supply and are installed in location.","2021-06-01T23:59:35","MOJO210085","Completed","2021-05-12T23:59:35","No","No","No","Internal","Is both gripes wire having any damage at present. What precautions/corrective action has been taken till new gripe wires will be supplied to vessel."]
[null,null,null,18717,null,"93_18/4/2021 7:04:04 AM","2021-04-05T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Glass portholes of the lifeboat have plenty  water marks.","LSA / FFA","Safety / LSA / FFA","External Factors","","","","","Lifeboat glass portholes cleaned thoroughly with soft emery paper. Varnish will be applied once supplied and requisition for the same is raised in deck stores.","2021-07-01T23:59:35","MOJO210089","Completed","2021-04-25T23:59:35","No","No","No","Internal","We will arrange to supply at port of call."]
[null,null,null,18718,null,"93_16/4/2021 3:26:58 PM","2021-04-07T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Noticed that the ME LO has water content almost 1 % as per shore LO analysis .","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related,Inappropriate Procedure","","","","","LO purifier& heater recently cleaned , now water content less than 0.2 . Planning to land again 3 monthly samples this port , WIO sensor recieved & fitted . ME LO purifier heater cleaned , now ME LO temperature reached 90 degrees for good purification when ME running ","2021-04-30T23:59:35","","Completed","2021-06-01T23:59:35","No","No","No","Internal","Vsl to clean steam side of ME LO purifier heater to achieve high LO inlet temperature to have better results."]
[null,null,null,18719,null,"93_18/4/2021 6:57:50 AM","2021-04-07T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Elevator wire last renewal date is not within last 05 yrs and the vessel has no spare on board.","Accommodation","Safety / LSA / FFA","Equipment Related","","","","","At suitable opputunity port call, tecnician will renew thw elevator wire","2021-09-01T23:59:35","MOJO210095","Completed","2021-09-10T23:59:35","No","No","No","Internal","Once wire on board, service team will be arranged for renewal of elevator wire."]
[null,null,null,18720,null,"93_16/4/2021 3:15:05 PM","2021-04-08T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","Noticed that the Ballast Pump No.1 has leak from its Mechanical seal","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","","","","","Ballast Pump No.1 has been overhauled . Job will be also reported as unplanned job for recoerds purpose in PAL ","2021-04-20T23:59:35","","Completed","2021-04-19T23:59:35","No","No","No","Internal","Vsl to update by mail once pump is  back to normal in addition to updating DDRL & raise RO for spares required for future use."]
[null,null,null,18721,null,"93_18/4/2021 6:33:04 AM","2021-04-09T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Stevedore's toilet WC unit found to be clogged and inoperational.","Accommodation","MLC Related","External Factors","","","","","As the commode was also broken & in bad condition , same replaced with new spare . The master control unit behind the commode & the water control valve changed , the old water control valve has been overhauled ","2021-04-30T23:59:35","","Completed","2021-04-20T23:59:35","No","No","No","Internal","Vsl to update by mail once job is completed."]
[null,null,null,18722,null,"93_16/4/2021 3:22:15 PM","2021-04-10T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Noticed that the AE LO purifier not working for a very long time on this vessel","E/R - Purifier","Eng. / Strg. Comp.","Equipment Related","","","","","Recently this job taken up . Opened up , cleaned purifier , rectified the defects , as the assembly Tested , found now ok , valve blocks ok , assembly done correctly , just the panel needs to be studies a bit to understand the codes ","2021-06-15T23:59:35","","Completed","2021-07-10T23:59:35","No","No","No","Internal","Vsl to try out & to revert with results. If spares required, RO to raise for it.. RO no to be updated in DDRL."]
[null,null,null,18724,null,"93_18/4/2021 6:29:05 AM","2021-04-10T23:59:35","Defect","Ship Staff","Ship Staff Insp.","After derusting the port side gangway several stanchions were found broken or cracked from the base. The collapsible railing also found to be holed.","Hull & Tanks","Cargo / Ballast Systems","External Factors","","","","","The cracked and broken stanchions repaired and installed back in location. The collapsible railing also repaired and installed back in location.","2021-04-20T23:59:35","","Completed","2021-04-15T23:59:35","No","No","No","Internal"]
[null,null,null,18723,null,"93_18/4/2021 9:44:43 AM","2021-04-12T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Small FO weeping was observed in No.09 CH aft bulkead (P) side, suspecting from No.1 VLSFO Tank port side and dried up.","Hull & Tanks","Cargo / Ballast Systems","External Factors","","","","","Temporarily the oil stain has been painted over. Cold repairs carried out during the voyage in Fuel oil tank. Permanent repairs to be carried out in the next dry dock. Defect added to Refman for Permanent repairs in Dry Dock.","2025-04-01T23:59:35","","Completed","2021-05-04T23:59:35","Yes","No","No","Internal","After making tank entry, pls raise defect in REFMAN with supporting drawings."]
[null,null,null,7587,null,"93_Tue Feb 12 2019 11:35:19 GMT+0000 (Coordinated Universal Time)","2021-04-19T23:59:35","Defect","Ship Staff","Ship Staff Insp.","All hatch coamings stiffeners on deck show heavy rusting","Deck - Pipe / Fittings","General Appearance","Equipment Related","","","","","Derusting & painting in progress.","2021-07-31T23:59:35","","Completed","2021-08-15T23:59:35","No","No","No","Internal","This observation is now more than 1.7 year old. Pls cancel this & re-raise if still need to be done as max time allowed for any observation to close is 3 months."]
[null,null,null,19602,null,"93_19/5/2021 6:57:06 AM","2021-05-05T23:59:35","Defect","Ship Staff","Ship Staff Insp.","It was seen that the No.1 VLSFO Bunker tank Port and Stbd side Vent head face plates were worn out and damaged. The vent head was covered with canvas cover to restrict the cargo dust from entering the tank.","Hull & Tanks","MARPOL Related","External Factors","","","","","The bunker tank vent head was completely derusted and face plates renewed with new ones. ","2021-05-12T23:59:35","","Completed","2021-05-07T23:59:35","No","No","No","Internal"]
[null,null,null,19597,null,"93_20/5/2021 7:51:19 PM","2021-05-15T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Lifeboat davit electric cable conduit pipe is holed. The junction box covers are also wasted.","LSA / FFA","Safety / LSA / FFA","External Factors","","","","","Cold repair carried out on the conduit pipe of lifeboat davit and junction box covers repaired.","2021-08-01T23:59:35","","Completed","2021-06-05T23:59:35","No","No","No","Internal"]
[null,null,null,19600,null,"93_20/5/2021 7:48:34 PM","2021-05-16T23:59:35","Observation","Ship Staff","Ship Staff Insp.","It was observed that the Lifeboat painter thimbles were rusted. The painter end was also worn out and the release mechanism was dry.","LSA / FFA","Emgcy. Systems","External Factors","","","","","Thimble derusted and painted, section of painter renwed and the release mechanism thoroughly lubricated.","2021-06-01T23:59:35","","Completed","2021-06-01T23:59:35","No","No","No","Internal"]
[null,null,null,19599,null,"93_20/5/2021 7:38:36 PM","2021-05-17T23:59:35","Defect","Ship Staff","Ship Staff Insp.","After derusting the stbd side gangway several stanchions were found broken or cracked from the base. The collapsible railing also found to be holed.","Deck - Machinery","Safety / LSA / FFA","External Factors","","","","","The cracked and broken stanchions repaired and installed back in location. The collapsible railing also repaired and installed back in location.","2021-08-01T23:59:35","","Completed","2021-05-25T23:59:35","No","No","No","Internal"]
[null,null,null,19598,null,"93_20/5/2021 7:56:22 PM","2021-05-20T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Newly supplied MOB marker lifebuoy does not fit into the stowage crutch at the bridge wings.","LSA / FFA","Safety / LSA / FFA","External Factors","","","","","Stowage crutch  modified as required so as to have a comfortable stowing of the lifebuoy. New MOB Lifebuoy installed.","2021-08-01T23:59:35","","Completed","2021-05-28T23:59:35","No","No","No","Internal"]
[null,null,null,19601,null,"93_21/5/2021 12:50:02 AM","2021-05-21T23:59:35","Defect","Ship Staff","Ship Staff Insp.","During routine monthly inspection it was seen that the MOB marker light for port side is not working. Both MOB markers smoke trigger pins and crutch are heavily corroded. Expiry dates for both MOB markers are not visible.","LSA / FFA","Safety / LSA / FFA","External Factors","","","","","Requisition received and MOB installed.","2021-08-01T23:59:35","MOJO210124","Completed","2021-07-06T23:59:35","No","No","No","Internal"]
[null,null,null,19741,null,"93_02/06/2021 16:06:13","2021-05-24T23:59:35","Defect","Ship Staff","Ship Staff Insp.","It was seen that the fittings for emregncy light at the funnel had competely wasted and the light was hanging from the edge.","Miscellaneous","Emgcy. Systems","External Factors","","","","","Pipe and flange for emergency light renewed and fitted back in location.","2021-08-01T23:59:35","","Completed","2021-06-02T23:59:35","No","No","No","Internal"]
[null,null,null,19734,null,"93_3/6/2021 5:06:24 PM","2021-05-26T23:59:35","Breakdown,Defect","Ship Staff","Ship Staff Insp.","Both Fire Pumps ' Bottom Cover ' of the Casing have leaks , same repaired by Brazing but need to be replaced by new spare","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","","","","","Temporary repairs carried out, brazing done on bottom, upon receiving spares bottom cover will be replaced.","2021-08-20T23:59:35","MOJO210123","Completed","2021-09-10T23:59:35","No","No","No","Internal"]
[null,null,null,19735,null,"93_3/6/2021 4:39:58 PM","2021-05-29T23:59:35","Breakdown,Defect","Ship Staff","Ship Staff Insp.","ACONIS MIMIC PMS  Card is not working & not showing display ","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","Spare recieved , now ok ","2021-06-10T23:59:35","","Completed","2021-06-15T23:59:35","No","No","No","Internal"]
[null,null,null,19736,null,"93_02/06/2021 16:03:30","2021-06-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","It was observed that the Hatch cover control box cover and hinges for No.3 and No.6  had corroded and wasted. The covers could not be locked in location.","Cargo Mach.","Cargo / Ballast Systems","External Factors","","","","","Covers and hinges renewed and fixed in location.","2021-09-01T23:59:35","","Completed","2021-06-12T23:59:35","No","No","No","Internal"]
[null,null,null,19737,null,"93_3/6/2021 4:47:50 PM","2021-06-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","It is noted that LED migration of Tube lights in accomodation & ER is pending , however awaiting spares ( Lamp Holders which were wrongly recieved ) ","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related,External Factors","","","","","Spare lamp holders recieved , job already started ","2021-08-20T23:59:35","","Completed","2021-08-15T23:59:35","No","No","No","Internal"]
[null,null,null,19738,null,"93_3/6/2021 4:51:49 PM","2021-06-02T23:59:35","Defect","Ship Staff","Ship Staff Insp.","ER Funnel area Blower platform weathertight door packing is not sealing properly ","E/R - Pipes/ valves & fittings,Miscellaneous","Eng. / Strg. Comp.","Equipment Related,External Factors","","","","","Packing renewed, problem rectified.","2021-08-15T23:59:35","","Completed","2021-08-15T23:59:35","No","No","No","Internal"]
[null,null,null,19739,null,"93_3/6/2021 4:55:30 PM","2021-06-02T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Noticed that the Soot tank drain valve is stucked recently , need to overhaul check the valve ","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Valve eased up , now ok ","2021-06-15T23:59:35","","Completed","2021-07-10T23:59:35","No","No","No","Internal"]
[null,null,null,19740,null,"93_4/6/2021 9:46:31 AM","2021-06-04T23:59:35","Defect","Ship Staff","Ship Staff Insp.","While anchoring it was seen that one of the lugs of the common link had come off and dislocated from the location between No.2 and No.3 shackle.","Miscellaneous","Mooring","External Factors","","","","","Lug welded at location.","2021-09-04T23:59:35","","Completed","2021-09-16T23:59:35","No","No","No","Internal"]
[null,null,null,22082,null,"93_27/10/2021 11:16:39 AM","2021-06-26T23:59:35","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","\n\nRaise requsition for deck air compressor.\n\n","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related","","","","","\n\nReq  MOJO210175 raised in PAL\n\n","2021-10-30T23:59:35","MOJO210175\n\n","Completed","2021-08-09T23:59:35","No","No","No","Internal"]
[null,null,null,22083,null,"93_27/10/2021 12:22:38 PM","2021-06-26T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Rudder angle indicator on bridge was deflected by 2 degree when wheel is at midship","Navigation - Others","Navigation","Equipment Related","","","","","Potentiometer renewed","2021-10-30T23:59:35","","Completed","2021-07-05T23:59:35","No","No","No","Internal"]
[null,null,null,22085,null,"93_27/10/2021 6:12:15 PM","2021-06-26T23:59:35","Critical Equipment","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Emergency Generator Radiator body to check , CW line to check","Critical Equip.","Safety / LSA / FFA","Equipment Related","","","","","Radiator body and cooling water line checked, found in good order.","2021-07-25T23:59:35","","Completed","2021-07-24T23:59:35","No","No","No","Internal"]
[null,null,null,22086,null,"93_27/10/2021 6:06:31 PM","2021-06-26T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Zener Barrier cables to follow up","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","Defective cable problem rectified.","2021-07-25T23:59:35","","Completed","2021-10-28T23:59:35","No","No","No","Internal"]
[null,null,null,22088,null,"93_27/10/2021 2:16:25 PM","2021-06-26T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Fire GS Overboard valve to clean & paint","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Valve derusted,greased up and painted","2021-07-25T23:59:35","","Completed","2021-07-05T23:59:35","No","No","No","Internal"]
[null,null,null,22089,null,"93_27 Oct 2021 1:48:00 PM","2021-06-26T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Order 01 pc big Gas meter as per GSM policy.","Miscellaneous","Safety / LSA / FFA","Equipment Related","","","","","Gas meter received at singapore on 17.10.2021","2021-10-20T23:59:35","MOJO210152","Completed","2021-10-17T23:59:35","No","No","No","Internal"]
[null,null,null,22090,null,"93_27 Oct 2021 2:13:09 PM","2021-06-26T23:59:35","Critical Equipment","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Both liferafts lashing is loose.","LSA / FFA","Safety / LSA / FFA","Human Error","","","","","BOTH LIFERAFT LASHING\n\nTIGHTENED.\n\n","2021-06-30T23:59:35","","Completed","2021-06-27T23:59:35","No","No","No","Internal"]
[null,null,null,22091,null,"93_27 Oct 2021 2:21:01 PM","2021-06-26T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","\n\nWinches render point marking pointers to be made of thicker plate.\n\n","Deck - Machinery","Mooring","Equipment Related","","","","","\n\nRENDER POINT MARKERS \n\nREPLACED WITH A THICKER \n\nPLATE POINTER.\n\n","2021-07-25T23:59:35","","Completed","2021-07-05T23:59:35","No","No","No","Internal"]
[null,null,null,22092,null,"93_27/10/2021 11:08:04 AM","2021-06-26T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Bunker davit hook missing safety latch.","Deck - Machinery","Safety / LSA / FFA","Equipment Related","","","","","\n\nSafety latch fitted in place\n\n","2021-07-25T23:59:35","","Completed","2021-07-08T23:59:35","No","No","No","Internal"]
[null,null,null,22093,null,"93_27/10/2021 11:10:46 AM","2021-06-26T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","\n\nFPk Store bilges to be dried & derusted & painted around.\n\n","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","Equipment Related","","","","","\n\nFPk Store bilges  dried & derusted & painted.\n\n","2021-07-25T23:59:35","","Completed","2021-07-04T23:59:35","No","No","No","Internal"]
[null,null,null,22094,null,"93_27/10/2021 11:13:55 AM","2021-06-26T23:59:35","Critical Equipment","Owner / Marine / Tech. Suptd.","Suptd. Insp.","\n\n\n\nSpare charges for portable fire extinguishers - Expiry stencil.\n\n","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","Spare charges for portable fire extinguishers - Expiry stencilled","2021-07-25T23:59:35","","Completed","2021-06-30T23:59:35","No","No","No","Internal"]
[null,null,null,22095,null,"93_27/10/2021 11:22:07 AM","2021-06-26T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","\n\nPort gangway air v/v wheel broken.\n\n","Deck - Machinery","Structural Condn. / WT integrity ","Equipment Related","","","","","\n\nWheel repaired and installed\n\n","2021-07-25T23:59:35","","Completed","2021-07-07T23:59:35","No","No","No","Internal"]
[null,null,null,22096,null,"93_27/10/2021 2:18:56 PM","2021-06-26T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Starboard Bilge well put pads","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","Pads removed.","2021-07-25T23:59:35","","Completed","2021-07-24T23:59:35","No","No","No","Internal"]
[null,null,null,22097,null,"93_27/10/2021 11:24:08 AM","2021-06-26T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","\n\nFwd life raft cradle to be derusted, senhouse slip renewed / straps to be renewed.\n\n","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","Cradle derusted, Senhouse slip\n\nand straps renewed.\n\n","2021-07-25T23:59:35","","Completed","2021-06-29T23:59:35","No","No","No","Internal"]
[null,null,null,22098,null,"93_27/10/2021 11:51:31 AM","2021-06-26T23:59:35","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Fwd lifejackets box lid & packing to be renewed.","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","Fwd lifejackets box lid deristed and painted & packing renewed.","2021-07-25T23:59:35","","Completed","2021-06-28T23:59:35","No","No","No","Internal"]
[null,null,null,22099,null,"93_27/10/2021 12:00:10 PM","2021-06-26T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","\n\nFwd winches gearcase sight glass painted.\n\n","Deck - Machinery","Mooring","Equipment Related","","","","","\n\nPAINT REMOVED FROM SIGHT\n\n GLASS AND HIGHLIGHTED.\n\n","2021-07-25T23:59:35","","Completed","2021-07-06T23:59:35","No","No","No","Internal"]
[null,null,null,22100,null,"93_27/10/2021 12:02:07 PM","2021-06-26T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","\n\nOil in drip trays to be cleaned, power packs FPk store.\n\n","Deck - Machinery","General Appearance","Equipment Related","","","","","Oil in drip trays to be cleaned, power packs FPk store.\n\n\n\nOil in drip trays cleaned\n\n","2021-07-25T23:59:35","","Completed","2021-06-29T23:59:35","No","No","No","Internal"]
[null,null,null,22101,null,"93_27/10/2021 12:04:00 PM","2021-06-26T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Rubber mat in front 220V panel in FPk store missing.","Elect. Mach. & Equip.","Safety / LSA / FFA","Equipment Related","","","","","Rubber mat in front 220V panel in FPk store installed.","2021-07-25T23:59:35","","Completed","2021-06-30T23:59:35","No","No","No","Internal"]
[null,null,null,22102,null,"93_27/10/2021 12:08:34 PM","2021-06-26T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Pressure gauges in windlass/winches power pack needles missing, tube leaking.","Deck - Machinery","Mooring","Equipment Related","","","","","\n\nMOJO210206 - PRESSURE GAUGES RAISED IN PAL, RECEIVED AT SINGAPORE, BOTH PRESSURE GAUGES RENEWED.LEAKED TUBE RENEWED.\n\n","2021-10-25T23:59:35","MOJO210206 ","Completed","2021-10-19T23:59:35","No","No","No","Internal"]
[null,null,null,22103,null,"93_27/10/2021 12:11:36 PM","2021-06-26T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Both gangway motor oil levels low, seal leaking.","Deck - Machinery","Structural Condn. / WT integrity ","Equipment Related","","","","","Both gangway motor oil drain out and renewed.Stbd side oil lvevel was high, oil drained up to normal level","2021-07-25T23:59:35","","Completed","2021-07-24T23:59:35","No","No","No","Internal"]
[null,null,null,22104,null,"93_27/10/2021 12:14:16 PM","2021-06-26T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Port lifeboat davit manual cranking handle stowing slot disfigured.","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","Port lifeboat davit manual cranking handle stowing slot renewed.","2021-07-25T23:59:35","","Completed","2021-07-01T23:59:35","No","No","No","Internal"]
[null,null,null,22105,null,"93_27/10/2021 12:16:37 PM","2021-06-26T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Provision crane oil tank gauge glass painted, chain barrier thinned down to be renewed.","Deck - Machinery","Structural Condn. / WT integrity ","Equipment Related","","","","","Gauge glass cleaned and paint\n\nremoved.\n\n","2021-07-25T23:59:35","","Completed","2021-07-05T23:59:35","No","No","No","Internal"]
[null,null,null,22106,null,"93_27/10/2021 12:30:37 PM","2021-06-26T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Foward and aft all mooring brake limit marking was sighted flexible, not permanent to avoid accidental shifting","Deck - Machinery","Mooring","Equipment Related","","","","","Foward and aft all mooring brake limit marking renewed with a thicker plate","2021-07-25T23:59:35","","Completed","2021-07-10T23:59:35","No","No","No","Internal"]
[null,null,null,22107,null,"93_27/10/2021 12:41:04 PM","2021-06-26T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Main Engine exhaust manifold cover shroud missing lagging pillow.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Lagging added for exhaust manifold","2021-07-25T23:59:35","","Completed","2021-07-05T23:59:35","No","No","No","Internal"]
[null,null,null,22108,null,"93_27/10/2021 12:44:53 PM","2021-06-26T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","\n\nNumerous manometers in E/R are dry.\n\n","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","FILLED WITH GLYCERINE WATER","2021-07-25T23:59:35","","Completed","2021-07-03T23:59:35","No","No","No","Internal"]
[null,null,null,22109,null,"93_27/10/2021 12:47:01 PM","2021-06-26T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","\n\nRags found tucked at many places on A/E.\n\n","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","Removed all rags from the all places","2021-07-25T23:59:35","","Completed","2021-06-27T23:59:35","No","No","No","Internal"]
[null,null,null,22110,null,"93_27/10/2021 12:54:29 PM","2021-06-26T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","A/E Jacket inlet thermometer painted over.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Renewed with spare thermometer","2021-07-25T23:59:35","","Completed","2021-07-03T23:59:35","No","No","No","Internal"]
[null,null,null,22111,null,"93_27/10/2021 12:56:10 PM","2021-06-26T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","\n\nEEBDs in E/R to be placed properly , with the pressure gauge visible upwards\n\n","LSA / FFA","Eng. / Strg. Comp.","Equipment Related","","","","","EEBDs in E/R to be placed properly , with the pressure gauge visible upwards","2021-07-25T23:59:35","","Completed","2021-06-28T23:59:35","No","No","No","Internal"]
[null,null,null,22112,null,"93_27/10/2021 12:57:58 PM","2021-06-26T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Portable foam monitor box, foam expiry date to be stenciled","LSA / FFA","Eng. / Strg. Comp.","Equipment Related","","","","","Expiry date stencilled.","2021-07-25T23:59:35","","Completed","2021-07-20T23:59:35","No","No","No","Internal"]
[null,null,null,22113,null,"93_27/10/2021 1:00:04 PM","2021-06-26T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Spare Ejector pump to be secured by wire rope & not ordinary rope","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","Completed, Secured by wire rope","2021-07-25T23:59:35","","Completed","2021-07-19T23:59:35","No","No","No","Internal"]
[null,null,null,22114,null,"93_27/10/2021 12:42:50 PM","2021-06-26T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","A/E No.02 T/C also missing lagging pillow.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","\n\nAdded new lagging around T/C\n\n","2021-07-25T23:59:35","","Completed","2021-07-05T23:59:35","No","No","No","Internal"]
[null,null,null,22115,null,"93_27/10/2021 12:33:30 PM","2021-06-26T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","MOT ladder on deck was found with heavy corrosion and deposit of rust","Deck - Machinery","Structural Condn. / WT integrity ","Equipment Related","","","","","MOT ladder on deck derusted and \n\npainted. Now looks new.\n\n","2021-07-25T23:59:35","","Completed","2021-07-22T23:59:35","No","No","No","Internal"]
[null,null,null,22116,null,"93_27/10/2021 1:02:57 PM","2021-06-26T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","\n\nFew Pressure switches on the Reefer machinery have their covers brittle , same to be covered by proper tin covers\n\n","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","Rectified with available spare.","2021-07-25T23:59:35","","Completed","2021-07-04T23:59:35","No","No","No","Internal"]
[null,null,null,22117,null,"93_27/10/2021 1:10:00 PM","2021-06-26T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","As LO Bunkering was in process so some LO tanks were gagged & noticed small drops , same to rectify","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","\n\nGag removed and rectified the leakage.\n\n","2021-07-25T23:59:35","","Completed","2021-07-07T23:59:35","No","No","No","Internal"]
[null,null,null,22118,null,"93_27/10/2021 1:12:21 PM","2021-06-26T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Aft Hydraulic panel lamp test shows some lamps need replacement","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","\n\nRequisition Raised(MOJO210159 ) and received at singapore on 17.10.2021,fused lambs renewed, now all found working satisfactory.\n\n","2021-07-25T23:59:35","MOJO210159","Completed","2021-10-24T23:59:35","No","No","No","Internal"]
[null,null,null,22119,null,"93_27/10/2021 1:13:59 PM","2021-06-26T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","1 spare motor in spare parts room to be labelled","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","\n\nLabelled the spare motor name\n\n","2021-07-25T23:59:35","","Completed","2021-07-07T23:59:35","No","No","No","Internal"]
[null,null,null,22120,null,"93_27/10/2021 1:15:53 PM","2021-06-26T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","\n\nGrey water retention line plan to be painted for easy identification by future crew\n\n","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Line painted and kept a notice for easy identification.","2021-07-25T23:59:35","","Completed","2021-07-01T23:59:35","No","No","No","Internal"]
[null,null,null,22121,null,"93_27/10/2021 1:18:12 PM","2021-06-26T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","DO settling tank manhole to be painted , few nuts to be fitted with washer to prevent any oil seep","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","TIGHTENED BY PLAIN WASHER AND PAINTED","2021-07-25T23:59:35","","Completed","2021-07-20T23:59:35","No","No","No","Internal"]
[null,null,null,22122,null,"93_27/10/2021 1:20:03 PM","2021-06-26T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","\n\nTo paint Purifier room bulkheads & save-alls\n\n","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","\n\nBulkheads and Savealls cleaned and painted.\n\n\n\n","2021-07-25T23:59:35","","Completed","2021-07-24T23:59:35","No","No","No","Internal"]
[null,null,null,22123,null,"93_27/10/2021 1:25:57 PM","2021-06-26T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","To paint floor of Funnel platforms upto Incinerator platform","Deck - Pipe / Fittings,Miscellaneous","Eng. / Strg. Comp.","External Factors","","","","","Funnel platform to Incinerator platform floor cleaned and painted.","2021-07-25T23:59:35","","Completed","2021-07-24T23:59:35","No","No","No","Internal"]
[null,null,null,22124,null,"93_27/10/2021 1:33:21 PM","2021-06-26T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Arrange DG spare Con rods , label the same","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Aux. Engine spare Con Rods arranged, covered and secured with label.","2021-07-25T23:59:35","","Completed","2021-07-25T23:59:35","No","No","No","Internal"]
[null,null,null,22125,null,"93_27/10/2021 1:37:35 PM","2021-06-26T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Area around Emergency air compressor ( Tween decks to paint both sides , P & S )","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related","","","","","Emergency Air Compressor soap washed and area near the same cleaned.","2021-07-25T23:59:35","","Completed","2021-07-21T23:59:35","No","No","No","Internal"]
[null,null,null,22126,null,"93_27/10/2021 1:40:29 PM","2021-06-26T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Area Starboard of Reefer compressor had some previous oil stains , same to paint","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","Area Starboard of Reefer compressor cleaned and painted","2021-07-25T23:59:35","","Completed","2021-07-25T23:59:35","No","No","No","Internal"]
[null,null,null,22127,null,"93_27/10/2021 1:31:24 PM","2021-06-26T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","AE LO purifier Block valves issue to be sorted & test the same","E/R - Purifier","Eng. / Strg. Comp.","Equipment Related","","","","","Sorted , now working good without vibrations .","2021-07-25T23:59:35","","Completed","2021-07-08T23:59:35","No","No","No","Internal"]
[null,null,null,22128,null,"93_27/10/2021 1:42:35 PM","2021-06-26T23:59:35","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","\n\nTo order spare AC compressor in future after discussion with Suptd\n\n","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","RO MOJO210008 raised & received at singapore on 17.10.2021","2021-07-25T23:59:35","","Completed","2021-10-17T23:59:35","No","No","No","Internal"]
[null,null,null,22129,null,"93_27/10/2021 1:45:17 PM","2021-06-26T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Boiler Feed Pump Lagging some places damaged , same to repair","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","\n\nDamaged lagging repaired.\n\n","2021-07-25T23:59:35","","Completed","2021-07-21T23:59:35","No","No","No","Internal"]
[null,null,null,22130,null,"93_27/10/2021 1:47:36 PM","2021-06-26T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Clean QCV lagging near LT Pumps areas","LSA / FFA","Eng. / Strg. Comp.","Equipment Related","","","","","\n\nQCV lagging near LT Pumps areas Cleaned.\n\n","2021-07-25T23:59:35","","Completed","2021-07-24T23:59:35","No","No","No","Internal"]
[null,null,null,22131,null,"93_27/10/2021 1:51:29 PM","2021-06-26T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","LT Pumps pressure gauges stains to remove","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","","","","","LT Pumps pressure gauges stains removed","2021-07-25T23:59:35","","Completed","2021-07-07T23:59:35","No","No","No","Internal"]
[null,null,null,22132,null,"93_27/10/2021 1:53:13 PM","2021-06-26T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","LT cooler No.1 has SW corrosion on some unions , same to rectify / paint","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Union renewed and area painted","2021-07-25T23:59:35","","Completed","2021-07-08T23:59:35","No","No","No","Internal"]
[null,null,null,22133,null,"93_27/10/2021 1:55:16 PM","2021-06-26T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","\n\nClean both MAC in area between compressor & motor coupling , paint saveall of all compressors\n\n","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related","","","","","\n\nCleaned all the area\n\n","2021-07-25T23:59:35","","Completed","2021-07-08T23:59:35","No","No","No","Internal"]
[null,null,null,22134,null,"93_27/10/2021 1:35:28 PM","2021-06-26T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","DG Units to stencil & wash paint all DG s","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","All Aux. Engine units stencilled on both side","2021-07-25T23:59:35","","Completed","2021-07-23T23:59:35","No","No","No","Internal"]
[null,null,null,22135,null,"93_27/10/2021 1:57:00 PM","2021-06-26T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ME Fuel Pumps Umbrella seal Glass covers to clean","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","ME Fuel Pumps Umbrella seal glass cover cleaned\n\n\n\n\n\n\n\n\n\n\n\n","2021-07-25T23:59:35","","Completed","2021-07-07T23:59:35","No","No","No","Internal"]
[null,null,null,22136,null,"93_27/10/2021 2:01:25 PM","2021-06-26T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","\n\nAir Bottle outlet valve stain to paint\n\n","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","\n\nStain cleaned and area painted.\n\n","2021-07-25T23:59:35","","Completed","2021-07-20T23:59:35","No","No","No","Internal"]
[null,null,null,22137,null,"93_27/10/2021 2:05:36 PM","2021-06-26T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Sludge Pump & Bilge Pump save all & area around to paint","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","","","","","Sludge Pump & Bilge Pump save all & area around  painted","2021-07-25T23:59:35","","Completed","2021-07-12T23:59:35","No","No","No","Internal"]
[null,null,null,22138,null,"93_27/10/2021 2:07:36 PM","2021-06-26T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Area below Blow down valve to paint","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Area below Blow down valve painted the area","2021-07-25T23:59:35","","Completed","2021-07-12T23:59:35","No","No","No","Internal"]
[null,null,null,22139,null,"93_27/10/2021 2:14:24 PM","2021-06-26T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Sewage overboard valve to clean","E/R - Pipes/ valves & fittings","General Appearance","Equipment Related","","","","","DERUSTED AND PAINTED","2021-07-25T23:59:35","","Completed","2021-07-24T23:59:35","No","No","No","Internal"]
[null,null,null,22140,null,"93_27/10/2021 2:21:11 PM","2021-06-26T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Expansion tank glass to clean","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","GLASS CLEANED AND PUT BACK","2021-07-25T23:59:35","","Completed","2021-07-07T23:59:35","No","No","No","Internal"]
[null,null,null,22141,null,"93_27/10/2021 2:23:59 PM","2021-06-26T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Clean Aft side various spring loaded valves , lubricate the same","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Cleaned and lubricated the same.","2021-07-25T23:59:35","","Completed","2021-07-06T23:59:35","No","No","No","Internal"]
[null,null,null,22142,null,"93_27/10/2021 2:26:44 PM","2021-06-26T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","\n\n220 V Insulation from Receptacles on deck to attend\n\n","Elect. Mach. & Equip.","Safety / LSA / FFA","Equipment Related","","","","","Rectified","2021-07-25T23:59:35","","Completed","2021-07-06T23:59:35","No","No","No","Internal"]
[null,null,null,22143,null,"93_27/10/2021 2:03:34 PM","2021-06-26T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Vacuum stripper line of Fire Pumps to ensure all clear","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Vacuum system overhauled and all lines cleared.","2021-07-25T23:59:35","","Completed","2021-07-04T23:59:35","No","No","No","Internal"]
[null,null,null,22144,null,"93_27/10/2021 2:28:46 PM","2021-06-26T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","\n\nAE#1, 2 & 3 - area between flywheel & AE end cover full of oil.\n\n","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","All AE'S flywheel area cleaned.","2021-07-25T23:59:35","","Completed","2021-07-08T23:59:35","No","No","No","Internal"]
[null,null,null,22145,null,"93_27/10/2021 5:51:09 PM","2021-06-26T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Both lifeboats self lowering wires to be recoiled properly in spool","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","SELF LOWERING WIRE \n\nCOMPLETELY UNCOILED AND \n\nRECOILED TIGHTLY\n\n","2021-07-25T23:59:35","","Completed","2021-07-05T23:59:35","No","No","No","Internal"]
[null,null,null,22146,null,"93_27/10/2021 5:54:55 PM","2021-06-26T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Galley, battery room, steering room exhaust fans mesh in poor condition, to be renewed.","Elect. Mach. & Equip.","Safety / LSA / FFA","Equipment Related","","","","","FABRICATION OF FRAME FOR MESH AND NEW MESH RENEWED.","2021-07-25T23:59:35","","Completed","2021-07-10T23:59:35","No","No","No","Internal"]
[null,null,null,22147,null,"93_27/10/2021 6:00:45 PM","2021-06-26T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Workshop machinery safety foot peddle to be modified as per Tech circular T-001-2021","Elect. Mach. & Equip.","Safety / LSA / FFA","Equipment Related","","","","","Completed,Workshop machinery foot peddle wiring modified as per Tech Circular T-001-2021","2021-07-25T23:59:35","","Completed","2021-07-24T23:59:35","No","No","No","Internal"]
[null,null,null,22148,null,"93_27/10/2021 6:03:07 PM","2021-06-26T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Flashback arrestor tags to be hanged showing the expiry date of the same","Elect. Mach. & Equip.","Safety / LSA / FFA","Equipment Related","","","","","Tag hanged along with expiry date","2021-07-25T23:59:35","","Completed","2021-07-10T23:59:35","No","No","No","Internal"]
[null,null,null,22149,null,"93_27/10/2021 6:09:52 PM","2021-06-26T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Grey water P side overboard line section to repair & then paint","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Pipeline repaired","2021-07-25T23:59:35","","Completed","2021-07-24T23:59:35","No","No","No","Internal"]
[null,null,null,22150,null,"93_27/10/2021 6:15:01 PM","2021-06-26T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Area behind WO tank to clean & paint that area including the tanks","E/R - Pipes/ valves & fittings","General Appearance","Equipment Related","","","","","WO tank area cleaned and painted","2021-07-25T23:59:35","","Completed","2021-07-22T23:59:35","No","No","No","Internal"]
[null,null,null,21903,null,"93_24/7/2021 9:49:43 AM","2021-06-26T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Several Drip tray plugs threads wasted","Deck - Pipe / Fittings","MARPOL Related","Equipment Related","","","","","All Drip tray plugs fabricated and installed with wire lashing.","2021-07-31T23:59:35","","Completed","2021-08-15T23:59:35","No","No","No","Internal"]
[null,null,null,21894,null,"93_24/7/2021 10:00:36 AM","2021-06-30T23:59:35","Non Conformity","Ship Staff","Ship Staff Insp.","Some extension boards are without surge protector or are made on board ","Elect. Mach. & Equip.","Safety / LSA / FFA","Equipment Related","","","","","MOJO210154 received at singapore on 17.10.2021, new extention boards with surge protector put in use.","2021-08-31T23:59:35","MOJO210154","Completed","2021-10-22T23:59:35","No","No","No","Internal","Required items will be suplied at next convenient port."]
[null,null,null,21904,null,"93_08/07/2021 20:43:41","2021-07-07T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Water seepage observed from No.6 Cargo hold forward bulkhead into the void space and finally into duct keel. ","Hull & Tanks","Cargo / Ballast Systems","External Factors","","","","","Carried out permanent repairs on both side of cracks by ‘v’ gouging the crack first, then multiple runs of welds, ie from CH No.6 side and void space No.5.","2021-10-06T23:59:35","","Completed","2021-07-26T23:59:35","No","No","No","Internal"]
[null,null,null,21905,null,"93_08/07/2021 20:47:18","2021-07-08T23:59:35","Defect","Ship Staff","Ship Staff Insp.","While derusting Access hatch of No.7 Cargo hold it was observed that the hinge of the cover was cracked. ","Cargo Mach.","General Appearance","External Factors","","","","","Access hatch cover dismantled, hinge welded and painted.","2021-10-07T23:59:35","","Completed","2021-07-30T23:59:35","No","No","No","Internal"]
[null,null,null,21906,null,"93_27/7/2021 9:42:12 PM","2021-07-23T23:59:35","Defect","Ship Staff","Engineering Audit","Main engine exhaust valve spring air pressure low alarm was popping up on AMS panel","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Local pressure gauge shown correct pressure, pressure switch calibrated, found malfunctioning,same renewed and problem rectified,no alarm on AMS panel","2021-07-23T23:59:35","MOJO210166","Completed","2021-07-23T23:59:35","No","No","No","Internal"]
[null,null,null,21907,null,"93_27/7/2021 9:50:29 PM","2021-07-24T23:59:35","Defect","Ship Staff","Ship Staff Insp.","During testing of Sewage holding tank high level alarm, alarm was not getting reset, float removed & inspected, found wasted ,corroded &   broken from its leg.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","Sewage holding tank high level alarm float renewed, alarm tried out working satisfactory","2021-07-25T23:59:35","","Completed","2021-07-25T23:59:35","No","No","No","Internal"]
[null,null,null,21895,null,"93_7/7/2021 3:54:44 AM","2021-07-26T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","It was noted that the starboard side bridge window glass has cracked.","Navigation - Others","Navigation","External Factors","","","","","Spare received and Bridge window glass renewed.","2021-10-07T23:59:35","MOJO210153","Completed","2021-10-28T23:59:35","No","No","No","Internal","Glass will be supplied to vsl during Singapore call"]
[null,null,null,21896,null,"93_18 Aug 2021 5:31:17 AM","2021-08-03T23:59:35","Defect","Ship Staff","Ship Staff Insp.","No.2 steering gear motor latching block malfuntioning,motor can not stop by push button","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","MOJO210167 Received onboard, latching block renewed.","2021-09-10T23:59:35","MOJO210167","Completed","2021-10-20T23:59:35","No","No","No","Internal","Spares will be supplied during SINGAPORE call in mid of Oct"]
[null,null,null,21898,null,"93_7 Sep 2021 12:10:34 AM","2021-08-24T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Galley cooking range 1 pc. hot plate in operational.","Miscellaneous","MLC Related","Equipment Related","","","","","RO MOJO210177 received at singapore on 17.10.2021, non operational hot plate renewed.","2021-10-10T23:59:35","MOJO210177","Completed","2021-10-23T23:59:35","No","No","No","Internal","Spares wwill be connected at next convenient port."]
[null,null,null,21908,null,"93_7 Sep 2021 12:16:19 AM","2021-08-30T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Emergency distribution panel 220 V(E2)magnetic contactor for emergency power is defective ","Elect. Mach. & Equip.","Emgcy. Systems","Equipment Related","","","","","RO MOJO210177 received at Tubarao on 07.09.2021, Magnetic contactor renewed & tried out, working satisfactory.","2021-10-10T23:59:35","MOJO210177","Completed","2021-09-09T23:59:35","No","No","No","Internal"]
[null,null,null,22084,null,"93_09/10/2021 03:52:32","2021-09-07T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Mooring lines get damaged because of the friction between fairlead and mooring line, caused of surging of vessel.","Miscellaneous","Mooring","Equipment Related","","","","","Anti-chafing received and used on mooring lines after berthing.","2021-12-31T23:59:35","MOJO210217 (Item No.1)","Completed","2021-11-07T23:59:35","No","No","No","Internal"]
[null,null,null,21899,null,"93_16 Sep 2021 9:54:40 PM","2021-09-09T23:59:35","Defect","Ship Staff","Ship Staff Insp.","ER vent fan starter panel MCCB & magnetic contactor defective ","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","Magnetic contactor received, renewed, fan tried out, working satisfactory.","2021-09-18T23:59:35","RO MOJO210097","Completed","2021-10-23T23:59:35","No","No","No","Internal","New MCB will be connected during vsl Singapore call."]
[null,null,null,21902,null,"93_02/10/2021 09:56:51","2021-09-09T23:59:35","Defect","Ship Staff","Ship Staff Insp.","CH.ENG and 3.ENG cabins porthole glass broken.","Accommodation","MLC Related","Equipment Related","","","","","Spare received and porthole glass replaced and renewed.","2021-11-29T23:59:35","MOJO210197","Completed","2021-10-28T23:59:35","No","No","No","Internal"]
[null,null,null,21900,null,"93_2/10/2021 9:24:04 AM","2021-09-10T23:59:35","Critical Equipment","Ship Staff","Ship Staff Insp."," Fore-peak tank WIAS is non-operational, Giving alarm continiously even if FPT is empty. \n\n• WIAS sensor protection pipe is having pin hole and some section of this pipe is badly corroded and wasted.\n\n• Water ingress sensor (anode type) is in damaged condition.","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","Equipment Related","","","","","1. Damaged section WIAS sensor protection pipe cropped, fabricated and renewed.                                                               2. New WIAS sensor tested and installed. ","2021-10-15T23:59:35","","Completed","2021-10-06T23:59:35","No","No","No","Internal","Vsl to carryout required repairs once tank is empty"]
[null,null,null,21901,null,"93_17/9/2021 10:19:48 AM","2021-09-14T23:59:35","Critical Equipment","Ship Staff","Ship Staff Insp.","Due to the age of the vessel and regular wear and tear it was observed that the Lifeboat top hatch hinges have been wasted, dogs look worn.","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","Spares received on 05.11.2021 at Zhoushan.                            Both lifeboat's top hatch and dog cleats renewed.","2021-12-15T23:59:35","MOJO210092","Completed","2021-11-10T23:59:35","No","No","No","Internal"]
[null,null,null,22087,null,"93_27/10/2021 4:02:55 PM","2021-09-25T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Aft hydraulic pump both pressure gauges needles missing\n\n","Deck - Mooring Machinery","Eng. / Strg. Comp.","Equipment Related","","","","","\n\nBoth pumps pressure gauges renewed..\n\n","2021-10-25T23:59:35","","Completed","2021-10-22T23:59:35","No","No","No","Internal"]
[null,null,null,22081,null,"93_27/10/2021 4:00:10 PM","2021-10-23T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Main engine unit 3 exhaust gas temperature sensor malfunctioning, giving false alarm","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Unit 3 sensor renewed at anchorage with newly received sapres.","2021-10-30T23:59:35","","Completed","2021-10-28T23:59:35","No","No","No","Internal"]
[null,null,null,23032,null,"93_17/11/2021 12:04:09 PM","2021-11-16T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Various cargo hold natural vent's louvers are in damaged condition. ","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","Equipment Related","","","","","All damaged natural vents cropped, fabricated and renewed.                   ","2022-01-31T23:59:35","","Completed","2021-12-07T23:59:35","No","No","No","Internal"]
[null,null,null,23034,null,"93_17/11/2021 12:10:44 PM","2021-11-16T23:59:35","Defect","Ship Staff","Ship Staff Insp.","CH No.4 (Port & aft) drain pipe NRV is wasted. ","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","Equipment Related","","","","","Drain pipe of CH No.4 cropped, fabricated and renewed. ","2021-11-28T23:59:35","","Completed","2021-11-28T23:59:35","No","No","No","Internal"]
[null,null,null,23388,null,"93_3/12/2021 6:00:13 PM","2021-11-18T23:59:35","Non Conformity","Ship Staff","Ship Staff Insp.","MUCKING WINCH HOOK DOES NOT HAVE SAFETY LATCH","Miscellaneous","Safety / LSA / FFA","Equipment Related","","","","","Mooring wiches Safety latchs fabricated and installed.","2021-12-30T23:59:35","","Completed","2021-12-28T23:59:35","No","No","No","Internal"]
[null,null,null,23389,null,"93_21/12/2021 5:34:31 AM","2021-11-21T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Port side grey water line section pipe pin hole","Deck - Pipe / Fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Section pipe removed from place , new pipe fabricated and fitted in place.","2021-12-30T23:59:35","","Completed","2021-12-23T23:59:35","No","No","No","Internal"]
[null,null,null,23384,null,"93_3 Dec 2021 12:15:40 PM","2021-12-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Engine room AMS ROS 1 hanged, DPS logger is getting stopped and operating station is not returning to normal working condition","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","kONGSBERG technician attended the vessel and resolved issue. CPU of ROS 1 taken shore for software installation and brought back to vessel, fitted back, working satisfactory.","2022-03-01T23:59:35","","Completed","2022-01-20T23:59:35","No","No","No","Internal","Makers tech arranged for attendance at Korea on 19th Jan'22."]
[null,null,null,23385,null,"93_15/12/2021 3:41:36 PM","2021-12-01T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Mooring winch's  clutch hard to engage,due to the short lenght of clutch shifting handle.","Deck - Mooring Machinery","Mooring","Equipment Related","","","","","Clutch shifting handle's length to be extended for All mooring wiches handles  fabricated and installed.","2022-03-31T23:59:35","","Completed","2022-01-10T23:59:35","No","No","No","Internal"]
[null,null,null,23395,null,"93_15/12/2021 3:46:39 PM","2021-12-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Hawse pipe (Port, Stbd) cover's foundation plate buckled up .","Deck - Pipe / Fittings","ISPS Related","Equipment Related","","","","","Hawse pipe (Port & Stbd) cover's foundation plates fabricated and installed.","2021-12-25T23:59:35","","Completed","2021-12-21T23:59:35","No","No","No","Internal"]
[null,null,null,23390,null,"93_21/12/2021 5:11:58 AM","2021-12-08T23:59:35","Defect","Ship Staff","Ship Staff Insp.","No.2 Provision reefer, plant main magnetic contactor fiund seized due to ageing.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","Main magnetic contactor renewed, tried out working satisfactory","2021-12-10T23:59:35","","Completed","2021-12-08T23:59:35","No","No","No","Internal"]
[null,null,null,23391,null,"93_15/12/2021 4:22:27 PM","2021-12-10T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Auxiliary engine water leakages into the combustion space through fuel injector nozzle holder and injector o'ring.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Water leakages have been rectified by identifying induvidual units and o'rings replacement carried out, RO MOJO210258 received onboard on 01/01/20222.New o,rings will be used for future routines on Auxiliary engines. ","2021-12-20T23:59:35","MOJO210258","Completed","2022-01-01T23:59:35","No","No","No","Internal"]
[null,null,null,23386,null,"93_15/12/2021 4:24:30 PM","2021-12-11T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Composite Boiler no.2  feed water pump  wear rings, impellers, casing worn out , cause of motor drive end bearing housing wear, due to imbalance its shaft bend","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","","","","","Pump overhauled with new shaft and mechanicals seal, casing ring, tried out running satisfactory","2022-03-10T23:59:35","MOJO210138","Completed","2022-12-07T23:59:35","No","No","No","Internal"]
[null,null,null,23392,null,"93_21/12/2021 4:53:23 AM","2021-12-12T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Composite boiler port side gauge glass leaking from gasket","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","Port side gauge glass dismantled and found gasket found broken, gauge glass gaskt renewed and boxed back. Trie dout no leakages observed.","2021-12-15T23:59:35","","Completed","2021-12-12T23:59:35","No","No","No","Internal"]
[null,null,null,23393,null,"93_15/12/2021 3:32:28 PM","2021-12-14T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Air Horn Pipe found  damaged on compass deck.","Navigation - Others","Navigation","Equipment Related","","","","","Damaged portion of the pipe has been cropped, fabricated  and renewed.","2021-12-20T23:59:35","","Completed","2021-12-16T23:59:35","No","No","No","Internal"]
[null,null,null,23394,null,"93_21/12/2021 5:22:11 AM","2021-12-20T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Composite boiler emergency feed line inlet valve bonnet water leakage","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","Valve bonnet removed from place and gasket renewed, tried out no leakages observed","2021-12-20T23:59:35","","Completed","2021-12-20T23:59:35","No","No","No","Internal"]
[null,null,null,24614,null,"93_01/02/2022 09:19:22","2021-12-23T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Ch No.2  Vertical ladder lowest platform flat bar  railing damaged from one side.","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","Equipment Related","","","","","Damaged part to be croped  and new bar to be fabricated.","2022-04-22T23:59:35","","Completed","2022-02-14T23:59:35","No","No","No","Internal"]
[null,null,null,24615,null,"93_01/02/2022 09:25:08","2021-12-23T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Ch No.3 Vertical ladder lowest platform railing damaged ","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","Equipment Related","","","","","Damaged railing to be roped and new to be fabricated","2022-04-22T23:59:35","","Completed","2022-02-11T23:59:35","No","No","No","Internal"]
[null,null,null,23387,null,"93_5/1/2022 5:43:12 AM","2021-12-31T23:59:35","Critical Equipment","Ship Staff","Ship Staff Insp.","Steering gear no.2 motor not stopping and changing over to high mode by push button switch","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","Found the problem in panel through redundancy circuit fuse, low run starting auxiliary relay got energized and pump was satrting. Fuse removed and system started working normal","2022-03-30T23:59:35","","Completed","2022-01-15T23:59:35","No","No","No","Internal"]
[null,null,null,23509,null,"93_15/1/2022 11:58:44 AM","2022-01-15T23:59:35","Defect","Ship Staff","Suptd. Insp.","Boiler feed water pump no.2 motor bearing housing worn out","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","","","","","New motor recived and renewed.","2022-03-15T23:59:35","MOJO220025","Completed","2022-01-28T23:59:35","No","No","No","Internal"]
[null,null,null,23033,null,"93_22 Nov 2021 8:50:55 AM","2022-01-27T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Control air dryer starter capacitor leaked off,dryer is in non operational condition. To install new control air dryer","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","New Control air dryer installed and put in use.","2022-04-27T23:59:35","","Completed","2022-03-04T23:59:35","No","No","No","Internal","Pls revert how control air health being maintained due to failure of dryer"]
[null,null,null,24613,null,"93_1/3/2022 3:13:24 PM","2022-02-27T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Gangway Turntable (top platform),bend about 15mm and upper platform shaft is slightly bend and getting stuck in shaft holderat approx 10 deg. from the horizontal position.","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","Equipment Related","","","","","Turn table has been repaired. Vessel recieved the required materials for top plateform. Job carried out during good weather condition on 9,10, & 13 May 2022. \nRepairs on port side Gangway upper platform completed; tried out and in order. ","2022-05-27T23:59:35","MOJO220056","Completed","2022-05-13T23:59:35","No","No","No","Internal","Vsl has already carried out repairs, pls revert what material from RO 220056 is required."]
[null,null,null,24639,null,"93_16/3/2022 2:38:23 AM","2022-03-10T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Oil Leakage from Speed control lever of port windlass ","Deck - Mooring Machinery","Mooring","Equipment Related","","","","","O ring & seals renewed & leakage rectified.","2022-06-10T23:59:35","","Completed","2022-03-15T23:59:35","No","No","No","Internal"]
[null,null,null,24638,null,"93_23 Mar 2022 7:39:44 AM","2022-03-15T23:59:35","Defect","Ship Staff","Ship Staff Insp.","AMS panel is having active alarm with -ve reading for Boiler F.O inlet pressure.","E/R - Boiler,E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Trouble shooting carried out and found that pressure transmitter is defective. New pressure transmitter received and fitted in place. Function of pressure transmitter and alarm tested found working satisfactory.","2022-07-14T23:59:35","RO: MOJO220063","Completed",null,"No","No","No","Internal","Spares will be supplied at next convenient port."]
[null,null,null,25300,59045,"93_Tue May 17 2022 11:24:12 GMT+0800","2022-03-23T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Main Engine Cylinder oil tank No.1, out valve found not holding.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Tank emptied and outlet valve renewed.","2022-06-22T23:59:35","","Completed","2022-05-09T23:59:35","No","No","No","Internal"]
[null,null,null,25293,58675,"93_Sat Apr 30 2022 10:46:56 GMT+0800","2022-04-02T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Amprer meter of Hyd hatc covers pumps showing incorrect readings.","Deck - Machinery","Eng. / Strg. Comp.","Equipment Related","","","","","Ampere meter checked against clamp meter and found to be defective. These need replacement. Spare ampere meter received replaced. Both Amp meter working satisfactory.","2022-07-01T23:59:35","MOJO220084","Completed","2022-04-30T23:59:35","No","No","No","Internal"]
[null,null,null,25294,34992,"93_Sun May 01 2022 15:27:31 GMT+0800","2022-04-04T23:59:35","Observation","Ship Staff","Ship Staff Insp.","STBD life boat battery is temporary replaced with used battery from emergency generator.","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","New battery received and fitted in place. Life boat engine starting tested found starting satisfactory. ","2022-07-03T23:59:35","STBD life boat battery is temporary replaced with used battery from emergency generator.","Completed",null,"No","No","No","Internal"]
[null,null,null,25295,22047,"93_Sun May 01 2022 15:33:22 GMT+0800","2022-04-14T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Cargo hold no 6 hatch cover fwd port side (outer) hydraulic cylinder jacking up operation in slow motion.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","Hydraulic cylinder jack renewed. ","2022-05-13T23:59:35","","Completed","2022-04-21T23:59:35","No","No","No","Internal"]
[null,null,null,25296,73664,"93_Sun May 01 2022 15:35:46 GMT+0800","2022-04-20T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Installation of deck air compressor is pending.","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related","","","","","Installation completed and deck air compressor put in use. ","2022-07-19T23:59:35","MOJO220090: MCCB FOR DECK AIR COMPRESSOR INSTALLATION\nMOJO220091 : AIR BOTTLE FOR DECK AIR COMPRESSO","Completed","2022-05-09T23:59:35","No","No","No","Internal"]
[null,null,null,25301,50941,"93_Fri Apr 29 2022 14:04:13 GMT+0800","2022-04-22T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Boiler low low shut down level float switch found not working.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","Float switch removed and dismantled, microswitch found malfunctioning. Same has been repaired and fitted back. Low low shut down of boiler tested and found working satisfactory.","2022-07-21T23:59:35","","Completed","2022-04-27T23:59:35","No","No","No","Internal"]
[null,null,null,25297,34907,"93_Tue May 17 2022 11:10:09 GMT+0800","2022-05-03T23:59:35","Defect,Observation","Ship Staff","Ship Staff Insp.","Aux engine F.O supply pump found leaking from the mechanical seal.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","","","","","Pump overhauled. Mechanical seal and other consumable parts renewed. Pump tested found working satisfactory. No leakage observed.","2022-08-02T23:59:35","","Completed","2022-05-05T23:59:35","No","No","No","Internal"]
[null,null,null,25298,92036,"93_Tue May 17 2022 11:19:07 GMT+0800","2022-05-07T23:59:35","Defect","Ship Staff","Ship Staff Insp.","On weekly routine found Sewage holding tank high level alarm not working.","Elect. Mach. & Equip.,E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Alarm float checked and found that float has been broken due to corrosion. Float replaced with new spare. Alarm tested found working satisfactory.","2022-08-06T23:59:35","","Completed","2022-05-07T23:59:35","No","No","No","Internal"]
[null,null,null,25302,47171,"93_Tue May 17 2022 11:27:47 GMT+0800","2022-05-07T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Both ballast pump discharge valve position indicator in ballast control room observed to be incorrect w.r.t actual valve position.","Deck - Machinery,E/R - Pipes/ valves & fittings","Cargo / Ballast Systems","Equipment Related","","","","","Valve position indicator potentiometer adjusted and offset in position indication removed. Now showing correct position.","2022-08-06T23:59:35","","Completed","2022-05-14T23:59:35","No","No","No","Internal"]
[null,null,null,25299,27595,"93_Tue May 17 2022 11:21:36 GMT+0800","2022-05-09T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Boiler feed water pump #1 found water leaking from the mechanical seal.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","","","","","Pump overhauled. Mechanical seal renewed. Pump tested found working satisfactory. No leakage observed.","2022-08-08T23:59:35","","Completed","2022-05-10T23:59:35","No","No","No","Internal"]
[null,null,null,null,43139,"93_Wed May 18 2022 07:46:54 GMT+0800","2022-05-13T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Leakages in four sections of deck air line on main deck","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","Equipment Related","","","","","All four sections of holed deck air line's renewed.","2022-06-13T08:00:00","","Completed","2022-05-22T08:00:00","No","No","No","Internal","Pls update during daily work done report."]
[null,null,null,null,85870,"93_Sun May 01 2022 15:35:13 GMT+0800","2022-04-14T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Cargo hold no 9 not closing due to misalignment of hatch cover chain mechanism.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","Cargo hold chain adjusted. Cargo hatch cover chain mechanism tried out and found satisfactory.","2022-07-13T08:00:00","","Completed","2022-05-28T08:00:00","No","No","No","Internal","Vsl to carryout this job on earliest as target date is falling due."]
[null,null,null,null,23861,"93_Tue Jun 07 2022 07:16:40 GMT+0800","2022-06-02T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Sewage holding tank overboard valve not functioning properly ","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","sewage holding overboard valve replaced with a spare one. valve tried/tested working satisfactory ",null,"","Completed","2022-06-04T08:00:00","No","No","No","Internal"]
[null,null,null,null,29532,"93_Tue Jun 07 2022 07:25:13 GMT+0800","2022-05-29T08:00:00","Breakdown","Ship Staff","Ship Staff Insp.","Incinerator primary burner motor found noisy ","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Incinerator burner Motor overhauled observed damaged bearing, new bearing installed. system tried out found satisfactory",null,"","Completed","2022-05-29T08:00:00","No","No","No","Internal"]
[null,null,null,null,65291,"93_Thu Jun 16 2022 06:13:11 GMT+0800","2022-06-13T08:00:00","Observation","Ship Staff","Ship Staff Insp.","Steam/water leaking from the flange ( bunker Tank heating coil condensate return pipeline ) due to damage/wear-out gasket .","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","There is no isolation valve in the pipeline- with taking all control measures Damaged gasket was renewed. ","2022-06-13T08:00:00","","Completed","2022-06-13T08:00:00","No","No","No","Internal"]
[null,null,null,null,66712,"93_Thu Jun 16 2022 06:21:28 GMT+0800","2022-06-06T08:00:00","Breakdown","Ship Staff","Ship Staff Insp.","while carrying out an internal inspection of the incinerator found refractory was fallen down in several places. In most places metal part is visible.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Cleaned the damaged area, and repatched the area with refractory materials ","2022-06-07T08:00:00","","Completed","2022-06-07T08:00:00","No","No","No","Internal"]
[null,null,null,null,65089,"93_Thu Jun 16 2022 06:28:03 GMT+0800","2022-06-08T08:00:00","Defect","Ship Staff","Ship Staff Insp."," incinerator flame failure alarm appears. upon investigation found that incinerator impeller vanes were broken/missing","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","The incinerator impeller was refabricated by ship staff from the galvanised plate. requisition raised ","2022-06-08T08:00:00","","Completed","2022-06-08T08:00:00","No","No","No","Internal"]
[null,null,null,null,31474,"93_Thu Jun 16 2022 07:00:03 GMT+0800","2022-06-15T08:00:00","Observation","Ship Staff","Ship Staff Insp.","During daily routine round found that seawater pump no 1  suction side pipe developed a hole (Approx. 4 mm Dia).on welding rim flange area","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","As seawater inlet and outlet valve not holding. hole plugged and cold work putty patch is applied on the all-around welding rim area","2022-06-15T08:00:00","","Completed","2022-06-15T08:00:00","No","No","No","Internal"]
[null,null,null,null,72896,"93_Thu Jun 16 2022 06:20:57 GMT+0800","2022-06-09T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Leakages in three sections of fire line at forward of cargo hold no 6 on main deck ","Deck - Pipe / Fittings","Safety / LSA / FFA","Equipment Related","","","","","Fabrication & Renewal of Fire line (3 sections) at fwd of ch no 6 completed. ","2022-06-30T08:00:00","","Completed","2022-06-16T08:00:00","No","No","No","Internal"]
[null,null,null,null,67476,"93_Tue Jun 07 2022 06:01:49 GMT+0800","2022-06-05T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Two hydraulic jack of cargo holds leaking from purging point.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","Both Hydraulic jack O-ring renewed.","2022-07-04T08:00:00","","Completed","2022-06-28T08:00:00","No","No","No","Internal"]
[null,null,null,null,44307,"93_Thu Jun 16 2022 06:35:52 GMT+0800","2022-06-15T08:00:00","Defect","Ship Staff","Ship Staff Insp.","HFO purifier no 2 Abnormally stop. upon investigation found that the vertical shaft roller bearing was seized and the belt was broken ","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","vertical shaft removed. removed seized bearing and replaced it with new bearing, shaft belt renewed. bowl cleaned.",null,"","Completed","2022-06-18T08:00:00","No","No","No","Internal"]
[null,null,null,null,96017,"93_Fri Jul 01 2022 14:14:59 GMT+0800","2022-06-16T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Boiler water feed pump no 1 re circulation line found various pin hole and leaking ","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","Fabricate new pipeline and put back in use ",null,"","Completed","2022-06-16T08:00:00","No","No","No","Internal"]
[null,null,null,null,51231,"93_Fri Jul 01 2022 14:25:13 GMT+0800","2022-06-19T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Galley hot plate no 2 giving low insulation(440V) and hot plate found not working at required temperature ","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","New spare hot plate installed and damaged hot plate cable completely renewed ",null,"","Completed","2022-06-19T08:00:00","No","No","No","Internal"]
[null,null,null,null,74086,"93_Fri Jul 01 2022 14:32:39 GMT+0800","2022-06-26T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Composite boiler feed water controller found not working/Not maintaining water level.upon investigation found diaphragm  damaged/cracked ","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","Damaged diaphragm replaced with spare new one . ",null,"","Completed","2022-06-26T08:00:00","No","No","No","Internal"]
[null,null,null,24635,null,"93_23 Mar 2022 7:35:30 AM","2022-03-11T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Main Engine F.O flowmeter not working.","E/R - Main Engine,E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Flow meter inspected and cleaned. tried repairing but it is not working. RO has been raised for new flow meter. Spare received at Durban 02-07-2022. flow meter installed ","2022-06-10T08:00:00","RO: MOJO220041","Completed","2022-07-05T08:00:00","No","No","No","Internal","Spares will be supplied at next convenient port."]
[null,null,null,null,35232,"93_Thu Jul 07 2022 15:48:07 GMT+0800","2022-07-05T08:00:00","Observation","Ship Staff","Ship Staff Insp.","Various leak/pin hole from fresh water pipeline in 3 sections in Purifier room \n","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","All three sections of fresh water leaky pipeline were removed and new \npipeline  fabricated and installed .","2022-07-07T08:00:00","","Completed","2022-07-07T08:00:00","No","No","No","Internal"]
[null,null,null,null,67509,"93_Sun May 01 2022 15:31:55 GMT+0800","2022-04-16T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Boiler cascade tank salinometer found not working.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Salinometer sensor dismantled and inspected, found to be damaged and not repairable.\nRO has been raised for the same.spare received at Durban 02-July-2022.\nnew spare salinometer installed .checked the working condition .found satisfactory","2022-07-15T08:00:00","MOJO220095: SALINITY CELL FOR BOILER CASCADE TANK","Completed","2022-07-06T08:00:00","No","No","No","Internal","Spares will be supplied at next convenient port."]
[null,null,null,null,45365,"93_Thu Jul 07 2022 20:53:47 GMT+0800","2022-07-07T08:00:00","Defect","Ship Staff","Ship Staff Insp.","The electric heater in the calorifier is not working and giving 440 low insulation. discovered the electric heater tube cracked/busted and the heating coils have come out","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Calorifier Electric heater replaced with new spare. working satisfactory ","2022-07-22T08:00:00","","Completed","2022-07-07T08:00:00","No","No","No","Internal"]
[null,null,null,24612,null,"93_12 Feb 2022 7:21:35 AM","2022-03-18T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Ballast pump #1, Ampere meter is showing offset reading and tested to be faulty. Same has to be renewed.","E/R - Pumps,Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","RO has been raised for The Ampere meter. spare received at Durban .defective ammeter  replaced with spare one ","2022-07-22T08:00:00","MOJO220039: AMMETER FOR BALLAST PUMP MOTOR","Completed","2022-07-08T08:00:00","No","No","No","Internal","Spares will be supplied at next convenient port."]
[null,null,null,24634,null,"93_23 Mar 2022 7:43:20 AM","2022-03-25T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Meat room temperature dia thermometer is found to be defective.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","spare received at Durban 02-July-2022. meat room thermometer replaced . found working satisfactory","2022-07-22T08:00:00","RO : MOJO220050","Completed","2022-07-08T08:00:00","No","No","No","Internal","Spares will be supplied at next convenient port."]
[null,null,null,24616,null,"93_12 Feb 2022 2:55:41 AM","2022-03-30T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Aft Hydraulic power pack, low oil level senosor is found to be not working. Same has to be renewed.","Deck - Mooring Machinery","Eng. / Strg. Comp.","Equipment Related,Human Error","","","","","spare received at Durban 02-07-2022. aft hydraulic power pack low oil sensor replaced with spare new one ","2022-06-29T08:00:00","MOJO220034 :LOW LEVEL SHUT DOWN SENSOR FOR AFT HYD POWER PACK","Completed","2022-07-07T08:00:00","No","No","No","Internal"]
[null,null,null,24637,null,"93_13 Mar 2022 11:01:02 AM","2022-04-28T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Mooring winch Hydraulic block, counter balance valve cover is damaged and causing hydraulic oil leakage.","Deck - Mooring Machinery","Mooring","Equipment Related","","","","","spare received at Durban on 02-07-2022 . mooring winch hydraulic block counter balance cover replaced with spare one ","2022-07-27T08:00:00","MOJO220059","Completed","2022-07-12T08:00:00","No","No","No","Internal","Spares will be connected once ready."]
[null,null,null,null,58098,"93_Tue Jul 12 2022 20:04:50 GMT+0800","2022-07-11T08:00:00","Observation","Ship Staff","Ship Staff Insp.","Four sections of boiler feed water pipe line have holes and are thinning out. They need to be replaced.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","All four sections of the boiler water feed line were newly fabricated and replaced .","2022-07-12T08:00:00","","Completed","2022-07-12T08:00:00","No","No","No","Internal"]
[null,null,null,null,94615,"93_Thu Jul 14 2022 21:32:51 GMT+0800","2022-07-14T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Aux engine fuel oil supply pump no 2 .trips on overload ","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","","","","","The motor of the auxiliary engine fuel oil supply pump no. 2 was overhauled, and it was discovered that the driving side shaft bearing was damaged. A new motor bearing was installed. The pump was tested and found to be functional.","2022-07-20T08:00:00","","Completed","2022-07-14T08:00:00","No","No","No","Internal"]
[null,null,null,null,67637,"93_Thu Jun 30 2022 15:54:24 GMT+0800","2022-06-28T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Leakages in two sections of deck air line on main deck","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","","","","","Holed & thinned down both airline section's renewed. Now No leakage in Deck air line on main deck.","2022-07-28T08:00:00","","Completed","2022-07-06T08:00:00","No","No","No","Internal"]
[null,null,null,null,46259,"93_Thu Jun 30 2022 15:37:03 GMT+0800","2022-06-27T08:00:00","Defect","Ship Staff","Ship Staff Insp."," Pneumatic lines are covered with a guard Plates which are connected to the pipe support on main deck. Due to heavy swell and shipping sea’s the guard plate which was already thinned down due to corrosion got disconnected from pipe support and fell down on main deck. Also at some locations the guard plates deformed.","Deck - Pipe / Fittings","Cargo / Ballast Systems","External Factors","","","","","Fitting & fixing of U lamp on Pneumatic lines guard completed.","2022-07-27T08:00:00","","Completed","2022-07-08T08:00:00","No","No","No","Internal"]
[null,null,null,null,62310,"93_Wed Aug 03 2022 13:41:19 GMT+0800","2022-07-21T08:00:00","Observation","Ship Staff","Ship Staff Insp.","Atmospheric condenser- tube corroded and leaking ","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Atmospheric condenser replaced with spare new one .all gasket renewed and system tried out working satisfactory ","2022-07-30T08:00:00","","Completed","2022-07-21T08:00:00","No","No","No","Internal"]
[null,null,null,null,44945,"93_Wed Aug 03 2022 13:50:39 GMT+0800","2022-07-23T08:00:00","Observation","Ship Staff","Ship Staff Insp.","The inlet and return valves on the No. 3 port bunker tank steam line are  leaking. . upon investigation found valve gland damaged also spindle thinned down .need replacement ","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","The inlet and return valves on the No. 3 port bunker tank steam line replaced with spare new one and flange gasket renewed . ","2022-07-24T08:00:00","","Completed","2022-07-23T08:00:00","No","No","No","Internal"]
[null,null,null,null,13667,"93_Wed Aug 03 2022 13:56:45 GMT+0800","2022-07-25T08:00:00","Observation","Ship Staff","Ship Staff Insp.","One pipe section of the condensate return line from several tanks to the atmospheric condenser has numerous holes, is corroded, and is thinning.same need to be replace","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","pipe section fabricated and renewed .","2022-07-27T08:00:00","","Completed","2022-07-26T08:00:00","No","No","No","Internal"]
[null,null,null,null,50652,"93_Wed Aug 03 2022 14:10:33 GMT+0800","2022-07-23T08:00:00","Observation","Ship Staff","Ship Staff Insp.","waste oil tank steam inlet valve body found hairline crack and leaking from gland , while the steam return line had a hole and was thinned out.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","waste oil tank steam inlet valve replaced with spare new one and steam return line pipe section renewed ","2022-07-25T08:00:00","","Completed","2022-07-23T08:00:00","No","No","No","Internal"]
[null,null,null,null,80148,"93_Wed Aug 03 2022 21:23:33 GMT+0800","2022-07-16T08:00:00","Defect","Ship Staff","Ship Staff Insp.","forwards deck hydraulic machinery showing 440 v low insulation (0.5 M ohm)","Deck - Machinery","Eng. / Strg. Comp.","Equipment Related","","","","","Motor terminal box opened up, disconnected the source cable and megger test carried out. Found satisfactory. further the power cables on the starter panel was disconnected and insulation test carried out, Found that out of three one  cables showing low insulation. Further opened up all the conduit boxes on the deck and found that there was water ingress.  Also found that insulation for the cable was worn out due to movement of cables inside conduit box. Drained the water, Gave rubber packing for the cables and blowed down with the air.  ","2022-07-31T08:00:00","","Completed","2022-07-20T08:00:00","No","No","No","Internal"]
[null,null,null,null,68215,"93_Wed Aug 03 2022 21:32:45 GMT+0800","2022-07-17T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Sound powered phone found non functional. ","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","Upon inspection found that there was no supply voltage to the telephone. tracing out the control circuit, found that the fuse was blown for the control unit. Renewed the same and made system back to normal. ","2022-07-31T08:00:00","","Completed","2022-07-17T08:00:00","No","No","No","Internal"]
[null,null,null,null,40812,"93_Wed Aug 03 2022 21:41:11 GMT+0800","2022-07-22T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Galley oven found to be giving abnormal noise upon turning on. ","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","Inspected and found out that the Aux. contractors malfunctioning. Renewed the same and system made back to normal. Found working satisfactory.   ","2022-07-31T08:00:00","","Completed","2022-07-24T08:00:00","No","No","No","Internal"]
[null,null,null,null,83728,"93_Thu Aug 04 2022 00:28:17 GMT+0800","2022-07-27T08:00:00","Observation","Ship Staff","Ship Staff Insp.","Port lifeboat remote wire rigging post thinned down .","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","Port lifeboat thinned down remote wire rigging post fabricated and renewed.","2022-08-03T08:00:00","","Completed","2022-07-28T08:00:00","No","No","No","Internal"]
[null,null,null,null,43616,"93_Sat Aug 06 2022 01:01:49 GMT+0800","2022-08-05T08:00:00","Defect","Ship Staff","Ship Staff Insp.","The hook for the dough mixer on the galley dough maker machine is broken.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","Broken dough mixer hook weld and fixed with nut and bolt arrengement. System tried outfound operational  ","2022-08-31T08:00:00","","Completed","2022-08-05T08:00:00","No","No","No","Internal"]
[null,null,null,null,63537,"93_Sat Aug 06 2022 01:08:59 GMT+0800","2022-08-03T08:00:00","Defect","Ship Staff","Ship Staff Insp.","After investigating the purifier no. 1 bowl leak alarm, it was discovered that the vertical shaft lower bearing had seized. Also damaged the friction pad and vertical shaft belt, as well as the sliding bowl seal ring and other o-rings.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Purifier overhauled and cleaned,all o rings and seal rings replaced. The vertical shaft bearing and belt were replaced with spares. The motor pulley friction pad was replaced. The purifier was tested and determined to be functional.","2022-08-10T08:00:00","","Completed","2022-08-05T08:00:00","No","No","No","Internal"]
[null,null,null,null,77524,"93_Wed Aug 10 2022 01:32:08 GMT+0800","2022-08-04T08:00:00","Defect","Ship Staff","Ship Staff Insp.","On routine round found main engine unit no 4 and 6 thermometers found defective ","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Defective thermometer replaced with spare one found working operational ","2022-08-10T08:00:00","","Completed","2022-08-04T08:00:00","No","No","No","Internal"]
[null,null,null,null,96000,"93_Wed Aug 10 2022 01:37:58 GMT+0800","2022-08-09T08:00:00","Defect","Ship Staff","Ship Staff Insp.","AUX Engine No. 1 fuel oil supply pump motor discovered a minor noise. After overhauling the motor, it was discovered that the non-drive side bearing had been damaged.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","","","","","Both the driving and non-driving side bearings of the motor have been replaced with spares. The motor was boxed up, and the pump was tested and confirmed to be working.","2022-08-15T08:00:00","","Completed","2022-08-09T08:00:00","No","No","No","Internal"]
[null,null,null,null,16372,"93_Sun Aug 14 2022 15:11:45 GMT+0800","2022-08-01T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Forward Bosun store supply fan reported not starting. ","","Eng. / Strg. Comp.","Equipment Related","","","","","Upon inspection, found that the auxiliary contactor malfunctioning. Renewed the aux. contactor and the latching block. Problem rectified. Working satisfactory. ","2022-08-04T08:00:00","","Completed","2022-08-02T08:00:00","No","No","No","Internal"]
[null,null,null,null,83991,"93_Sun Aug 14 2022 15:22:00 GMT+0800","2022-08-03T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Elevator door found to be not closing. ","","Eng. / Strg. Comp.","Equipment Related","","","","","Upon inspection, found that the door closing relay was energizing and de-energizing every 3 seconds. Switched off the breaker, closed the door manually and carried out the reset procedure as mentioned in the handing over. The problem still exists. On further inspection, found that the sensors for the door open and close on the cable trunk were malfunctioning. Rectified the same. A system is put back to normal.  Working satisfactory. ","2022-08-08T08:00:00","","Completed","2022-08-05T08:00:00","No","No","No","Internal"]
[null,null,null,null,44341,"93_Sun Aug 14 2022 15:32:05 GMT+0800","2022-08-05T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Bilge pump found to be tripping on overload. ","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","","","","","Upon inspection, found that the terminal connection on the motor was loose and the clamping for belt drive cover broken. Fixed the same and tried out. Found running satisfactory.","2022-08-07T08:00:00","","Completed","2022-08-06T08:00:00","No","No","No","Internal"]
[null,null,null,null,52680,"93_Sun Aug 14 2022 15:46:12 GMT+0800","2022-08-11T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Forward mast starboard side flood light reported not working. ","Elect. Mach. & Equip.","Mooring","Equipment Related","","","","","Renewed the fused lamps. Found that upon switching on, the lamp got fused instantly. On further inspection, found that the terminals of the ballast unit for the flood light burnt out and one terminal of the capacitor was detached from the terminal due to burnout. Replaced the terminal strip and connected the capacitor. Tried out after replacing the lamp, found working in good order.   ","2022-08-14T08:00:00","","Completed","2022-08-12T08:00:00","No","No","No","Internal"]
[null,null,null,24636,null,"93_23 Mar 2022 7:48:07 AM","2022-03-25T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Forward mast Light fixture is found in damaged condition.","Deck - Pipe / Fittings,Elect. Mach. & Equip.","Structural Condn. / WT integrity ","Equipment Related","","","","","The damaged light fixture is replaced with the spare. function checked found operational .","2022-06-24T08:00:00","RO: MOJO220049","Completed","2022-08-01T08:00:00","No","No","No","Internal","Spares will be supplied at next convenient port."]
[null,null,null,null,74834,"93_Sun Aug 28 2022 18:36:21 GMT+0800","2022-08-24T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Main engine unit no.4 crosshead bearing temperature gave erratic reading.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Inspected and found that the sensor was defective. Renewed the temperature sensor with the spare onboard. Parameters monitored. Found to be in good order. ","2022-08-30T08:00:00","","Completed","2022-08-26T08:00:00","No","No","No","Internal"]
[null,null,null,null,34324,"93_Wed Aug 31 2022 03:10:16 GMT+0800","2022-08-26T08:00:00","Observation","Ship Staff","Ship Staff Insp.","Port and stbd side gangway railings Stanchions are seized and require hard pull to rig up.","Deck - Machinery","Safety / LSA / FFA","Equipment Related","","","","","Port and stbd side gangway railings Stanchions eye plates repaired and fixed back.  Stanchions are freely moving after repairs.","2022-08-30T08:00:00","","Completed","2022-08-30T08:00:00","No","No","No","Internal"]
[null,null,null,null,15072,"93_Wed Aug 31 2022 14:58:15 GMT+0800","2022-08-22T08:00:00","Defect","Ship Staff","Ship Staff Insp."," the vessel notices external water leakage from the cylinder cover cooling jacket while drifting Off Gibraltar. At the same time, the main engine scavenges drain tank high-level alarm sounded. Upon opening under the piston area found mist and slight water seepage from the liner to scavenge space area of the # 5 unit.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","\nNo. 5 cylinder head cover along with the cooling jacket removed. A crack detection test was carried out on the cylinder liner and cylinder cover, the crack was detected on the internal surface of the cylinder cover \nThe vessel replaced the damaged cylinder cover with a spare one along with the new cooling water jacket. Also replaced the exhaust valve with a spare, overhauled one with a new seal ring and O-ring. \nThe cylinder head is boxed up with proper hydraulic tightening. Cooling water opened up and no leaks were detected. The engine was tried out & found in good order.\n\n","2022-09-10T08:00:00","","Completed","2022-08-23T08:00:00","No","No","No","Internal"]
[null,null,null,null,86696,"93_Wed Aug 31 2022 15:04:12 GMT+0800","2022-08-26T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Condensate pipeline above cascade tank found leaking badly. \n","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Wasted pipeline removed from place after steam isolation and new pipeline with new flanges made. New one fitted and line made normal, checked for any leakage, satisfactory.","2022-10-01T08:00:00","","Completed","2022-08-26T08:00:00","No","No","No","Internal"]
[null,null,null,null,46326,"93_Wed Aug 31 2022 15:08:29 GMT+0800","2022-08-26T08:00:00","Defect","Ship Staff","Ship Staff Insp.","HFO purifier No.2 bowl was not closing, leaking continuously. Belt found broken. ","E/R - Purifier","Eng. / Strg. Comp.","Equipment Related","","","","","Purifier isolated and opened, upon the inspection, found sealing ring damaged, vertical shaft bearing seized and belt broken. O rings renewed, bearing renewed, belt renewed, friction pads renewed. water flow checked, ampere checked. The purifier started, working satisfactorily without any leakage.\n","2022-08-31T08:00:00","","Completed","2022-08-27T08:00:00","No","No","No","Internal"]
[null,null,null,null,79420,"93_Wed Aug 31 2022 15:19:27 GMT+0800","2022-08-29T08:00:00","Defect","Ship Staff","Ship Staff Insp.","A/E No 1 cooling water inlet pressure low alarm is activated, as well as noise and vibration observed from the A/E NO 1 cooling water pump.\n","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Immediately after receiving the alarm, A/E No 2 took on load and stopped A/E #1 . Opened cooling water pump assembly found that driven gear side claw washer and nut was missing/fallen down in sump, driven gear was got damaged as well as impeller shaft found bend. The sump oil was transferred to an empty drum and the sump was thoroughly cleaned and a magnet was used to remove any remaining metal particles in A/E no 1 sump. Cleaning of the L.O. filter was carried out along with L.O. cooler draining. Fresh oil is taken in AE#1 sump.  AE#1 damaged cooling water pump dismantled for overhaul. As the driven gear had got damaged as well as the impeller shaft had bent, Two used and discarded shafts were found, key slot and thread were damaged. Key slot made, and threads remade. One shaft made ready to use, after full assembly and torque tightness 150 bar according to manual instruction impeller found to be hard to rotate .disasembled pump and used another shaft, shaft found damaged in a key area, key area brought to the proper size. O ring, bearings and lip seal renewed, Pump assembled according to maker's instruction with the old cover. tried by rotation with a hand found smooth. the whole assembly was put back and the engine was tried out on idle to monitor the pump. pump building up the proper pressure of 3.2 bar. AE 1 taken on load, cooling water pump pressure is normal","2022-09-15T08:00:00","","Completed","2022-08-30T08:00:00","No","No","No","Internal"]
[null,null,null,null,93295,"93_Wed Aug 31 2022 16:46:55 GMT+0800","2022-08-16T08:00:00","Defect","Ship Staff","Ship Staff Insp.","The main engine exhaust gas outlet temperature of unit #4 was found to be giving out erratic readings. while local reading shows normal ","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Upon inspection, found that the temperature sensor was defective. Renewed the thermocouple. Even after the renewal, found that the problem still exists. On further inspection, found that the amplifier unit for the same was malfunctioning. Renewed the amplifier for the #4 unit. Zero and span adjustments were carried out. The system was put back to use and monitored, Working satisfactorily. ","2022-08-20T08:00:00","","Completed","2022-08-17T08:00:00","No","No","No","Internal"]
[null,null,null,null,97179,"93_Wed Aug 31 2022 17:01:35 GMT+0800","2022-08-19T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Auto telephone on bridge reported dial function is having error connecting to other lines. ","Elect. Mach. & Equip.","Communication","Equipment Related","","","","","Upon inspection, found that the dial PCB was defective. Replaced the dial PCB with the spare phone. Tried and tested. Dial function found working satisfactory but there was a disturbance in line. Renewed the cable for the handset and tried out. All working in good order.  ","2022-08-22T08:00:00","","Completed","2022-08-20T08:00:00","No","No","No","Internal"]
[null,null,null,null,96602,"93_Wed Jan 11 2023 16:11:48 GMT+0800","2023-01-10T08:00:00","Critical Equipment","Ship Staff","Ship Staff Insp.","water ingress alarm system faulty","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","WIA system attended by service engineer at Dry dock. All faults in the system rectified and system working satisfactorily","2023-02-22T08:00:00","","Completed","2023-01-20T08:00:00","No","No","No","Internal"]
[null,null,null,null,12319,"93_Thu Sep 15 2022 17:09:50 GMT+0800","2022-09-09T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Ballast pump valve control indication on Ballast control console not closing completely. ","Elect. Mach. & Equip.","Cargo / Ballast Systems","Equipment Related","","","","","Checked the valve condition for opening and closing locally by actuating from Ballast control console, found to be in good order. On further inspection, found that the Valve position indicator in VRCS cabinet was not making contact with the stop indication. Hence we carried out the fine adjustment as per manual by adjusting the scale angle corresponding with the actuator. Monitored the flow indicator disc for proper functioning of open and close indication. Corrected the error on ballast control console potentiometer. Tried and tested out, all found to in good order. ","2022-09-30T08:00:00","","Completed","2022-09-10T08:00:00","No","No","No","Internal"]
[null,null,null,null,11514,"93_Thu Sep 15 2022 20:53:15 GMT+0800","2022-09-01T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Starboard side Bilge shore discharge connection manifold pipeline found crack.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","starboard side bilge discharge  connection pipeline removed from place, new pipeline fabricated and fitted in starboard manifold with new gaskets.","2022-10-01T08:00:00","","Completed","2022-09-02T08:00:00","No","No","No","Internal"]
[null,null,null,null,37909,"93_Thu Sep 15 2022 21:06:38 GMT+0800","2022-09-06T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Bunker manifold drain valve found damaged","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Damaged drain valve removed , new valves fitted in place.","2022-10-06T08:00:00","","Completed","2022-09-06T08:00:00","No","No","No","Internal"]
[null,null,null,null,65074,"93_Thu Sep 15 2022 23:06:29 GMT+0800","2022-09-09T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Incinerator misfiring while try to fire on Diesel oil. ","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Burner routine carried out. Refractory checked, found in bad condition. Metal part visible ,Inside area cleaned and refractory patch up carried out. Air flow holes checked and cleared . Electrodes renewed and distance adjusted. Mixing disc renewed.  Incinerator burner put back and tried out, working satisfactory on diesel oil and sludge mode.please note that refractory patch up work carried out every around 10-15 days ","2022-10-31T08:00:00","","Completed","2022-09-12T08:00:00","No","No","No","Internal"]
[null,null,null,null,40229,"93_Thu Sep 15 2022 23:29:19 GMT+0800","2022-09-11T08:00:00","Defect","Ship Staff","Ship Staff Insp.","No.1 Main sea water pump suction pipeline line got holed.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","LT cooler isolated and connection made for sea water from emergency fire pump. Aux. engine cooling water temperature monitored.  Once confirmed that temperature got stable, Main sea water pump stopped and isolated. sea chest valve shut and isolated.  Holed pipeline removed from place, taken to workshop and hole area built up by welding. Epoxy coat applied on welding area. Pipeline fitted back into sea water pump suction side.  Sea chest purged and put in use. Sea water pump valve opened and purged, checked for any leakage. Pump started after confirming no leakages from pipe and pump side. LT cooler emergency fire pump connection removed and put back into normal  operation.","2022-09-30T08:00:00","","Completed","2022-09-14T08:00:00","No","No","No","Internal"]
[null,null,null,null,37992,"93_Wed Aug 31 2022 18:00:41 GMT+0800","2022-08-27T08:00:00","Defect","Ship Staff","Ship Staff Insp.","AFT ICCP showing current reading of 0 ampere. ","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","",""," Currently the system is in automatic mode.  In the aft I.C.C.P, the voltage is 1.2V, current is 0A, voltage of Ref1 & Ref2 electrodes are 160mV & 145mV respectively. The current reading of 0 ampere has been constant and has not changed at all. There is no alarm indication on the panel. we tried to reset the system by turning off the breaker and turning it on back. But the output is same.  Inspected the system for any signs of loose connection of the wiring or visual defects. Checked all the fuses, found in good condition.  The system looks healthy.  After seeking guidance from the technical department, we carried out complete system check which is as follows ; System panel turned OFF. Inspected panel securing bolts. Checked the condition of all the fuses. Checked the panel's internal wiring for any loose connections. Checked the mains input voltages, measured anode open circuit potential and resistance by removing the cable. Disconnected reference cell wires from panel terminals and measured the reference cell potentials and resistance, then reconnected the cables. Carried out manual mode checks by increasing the percentage output step by step. Carried out automatic mode checks and logged the readings from the panel from time to time as per the mail.  Log sheet has been forwarded to the technical department and was suggested that the system is in good condition and to run it in the automatic mode. ","2022-09-10T08:00:00","","Completed","2022-09-06T08:00:00","No","No","No","Internal"]
[null,null,null,null,94165,"93_Wed Aug 31 2022 17:56:00 GMT+0800","2022-08-16T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Steering gear #1 hydraulic oil level low alarm in active state","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","As the alarm was not getting reset, we checked the functioning of the float. NO, NC was functioning properly. checked the junction box in the steering gear room to which the float is connected, same NO NC was reflected. checked the terminal box under the steering gear starter panel, NO NC was reflected.  Further we inspected the DC annunciator alarm panel on bridge control console, found that the alarm was in active state. suspected the I/O card was defective and swapped the I/O card with the spare one. But the problem still exists. Further we removed the input cable(304) from the DC annunciator on bridge console and connected back. Alarm got reset. Tried out the functioning of the alarm several times by activating the float. Found working satisfactory. ","2022-09-10T08:00:00","","Completed","2022-09-02T08:00:00","No","No","No","Internal"]
[null,null,null,null,19534,"93_Mon Aug 15 2022 01:37:58 GMT+0800","2022-08-12T08:00:00","Observation","Ship Staff","Ship Staff Insp.","Hydraulic return branch line near No. 1 cargo hold aft Port side thinned down and causing small leakage.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","","","","","The hydraulic return branch line valve was closed and isolated. A new section of the pipeline fabricated and replaced with a damaged one. Hydraulic pump tried out and found no leakages.","2022-11-11T08:00:00","","Completed","2022-09-24T08:00:00","No","No","No","Internal"]
[null,null,null,null,99129,"93_Fri Sep 30 2022 16:11:05 GMT+0800","2022-09-23T08:00:00","Observation","Ship Staff","Ship Staff Insp.","Thinned down and rusted fire branch line section (3.5 mtrs ) Fwd of CH No. 2 port side.","Deck - Pipe / Fittings","Safety / LSA / FFA","Equipment Related","","","","","Thinned down fire branch line section(3.5 mtrs) removed. Fabricated new section and replaced with damaged one. Fire pump run and no leakage found.","2022-09-25T08:00:00","","Completed","2022-09-24T08:00:00","No","No","No","Internal"]
[null,null,null,null,68889,"93_Fri Sep 30 2022 16:55:14 GMT+0800","2022-09-15T08:00:00","Observation","Ship Staff","Ship Staff Insp.","Incinerator burner motor found not running. ","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","Burner motor opened up and found that the impeller was misaligned. Rectified the same and fixed back. Tried out and monitored the timers and relay. All working in good order. ","2022-09-18T08:00:00","","Completed","2022-09-16T08:00:00","No","No","No","Internal"]
[null,null,null,null,18983,"93_Fri Sep 30 2022 17:15:12 GMT+0800","2022-09-16T08:00:00","Defect","Ship Staff","Ship Staff Insp.","3 Numbers of Main engine cylinder head hydraulic jacks found leaking.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Defective hydraulic jacks opened up and inspected, found o rings damaged. Same renewed and jacks tried out. Working satisfactory without leak.","2022-09-18T08:00:00","","Completed","2022-09-16T08:00:00","No","No","No","Internal"]
[null,null,null,null,17132,"93_Fri Sep 30 2022 17:22:14 GMT+0800","2022-09-26T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Electric portable grinder reported non functional. ","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","Checked if the source cable are intact. Checked if the source voltage is being received at the cable end terminals. On further inspection, found that the carbon brushes are worn out. Replaced the same and tried out. Working satisfactory.  ","2022-09-30T08:00:00","","Completed","2022-09-26T08:00:00","No","No","No","Internal"]
[null,null,null,null,81387,"93_Fri Sep 30 2022 17:50:29 GMT+0800","2022-09-06T08:00:00","Defect","Ship Staff","Ship Staff Insp.","No.1 HFO Purifier driving belt found damaged while operation and purifier tripped.","E/R - Purifier","Eng. / Strg. Comp.","Equipment Related","","","","","No.1 HFO Purifier opened up. Disc stack, sliding bowl vertical shaft removed. Checked bearing condition. found normal. Sump cleaned. The damaged driving belt was renewed. bowl cleaned, sliding bowl o-ring renewd . HFO purifier tried out, working satisfactorily.","2022-09-30T08:00:00","","Completed","2022-09-09T08:00:00","No","No","No","Internal"]
[null,null,null,null,43059,"93_Fri Sep 30 2022 17:57:41 GMT+0800","2022-09-11T08:00:00","Defect","Ship Staff","Ship Staff Insp.","440V low insulation alarm triggered. ","Elect. Mach. & Equip.,Deck - Machinery","Eng. / Strg. Comp.","Equipment Related","","","","","Upon inspection found that the low insulation is from Hydroblaster. Opened up the terminal box, removed the cable terminals and megger test carried out for the motor,  found satisfactory. Further checked the insulation on the cable and found low insulation.  Renewed the cable. Reconnected the system and tried out. Alarm got reset.  Found working satisfactory.   ","2022-09-15T08:00:00","","Completed","2022-09-12T08:00:00","No","No","No","Internal"]
[null,null,null,null,81816,"93_Fri Sep 30 2022 18:02:24 GMT+0800","2022-09-18T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Duct keel exhaust fan motor foundation found damaged.","Deck - Pipe / Fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Duct keel exhaust fan motor foundation fabricated and motor boxed up.","2022-09-24T08:00:00","","Completed","2022-09-20T08:00:00","No","No","No","Internal"]
[null,null,null,null,85127,"93_Sun Oct 16 2022 04:26:02 GMT+0800","2022-10-04T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Waste Oil tank alarm not getting activated. ","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","Inspected the float for NO, NC by activating the float and releasing it. On further inspection, found that the timer was faulty. Renewed the timer and checked the functioning of float. System found working satisfactory. ","2022-10-08T08:00:00","","Completed","2022-10-05T08:00:00","No","No","No","Internal"]
[null,null,null,null,78038,"93_Sun Oct 16 2022 04:34:24 GMT+0800","2022-10-11T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Air handling unit motor running on less ampere in high mode and the draft was not sufficient to reach the accommodation. ","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","Checked the condition of the motor, found satisfactory.  Greased the impeller side. Checked the condition of the impeller , Found to be in good condition. Checked the condition of the V- belt and found that there were cracks. Renewed the V-belts. Adjusted the tightness. Checked the alignment. System put back to use and monitored the parameters and the draft. System working satisfactory.  Air con compressor cleaning carried out belt tension inspected and adjusted as necessary.","2022-10-13T08:00:00","","Completed","2022-10-12T08:00:00","No","No","No","Internal"]
[null,null,null,null,44714,"93_Sun Oct 16 2022 04:41:18 GMT+0800","2022-10-05T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Garbage compactor reported non-functional.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","Upon inspection, found that the cable was detached and the trippped  due to overload. Connected the cable back crimping with new lugs. Cable tightness checked. System put back to normal. Checked the direction of the motor, abnormal noise of motor and pump. Tried out on an empty load and checked if there is any leaking in the joints and sealings, functioning of the limit switch.  System working satisfactory.  ","2022-10-09T08:00:00","","Completed","2022-10-05T08:00:00","No","No","No","Internal"]
[null,null,null,null,70472,"93_Sun Oct 16 2022 04:44:14 GMT+0800","2022-10-04T08:00:00","Observation","Ship Staff","Ship Staff Insp.","During inspection the attached A/E # 1-Lub.oil. pump gear teeth and drive gear teeth found thinned down.\nThe pump was dismantled and a thorough inspection carried out, we found the L.O. pump gear thinned down and teeth profile changed. The same condition is found in the Aux. machinery#1- drive gear. When the gear was removed from the Lub oil pump, we found that the shaft key slot had widened and the shaft key, was Chamfer on one side and flattened. The driven gear for lub oil pump was slipping from the shaft. Lube oil pump gear locking nut was found on the shaft but loosened on a couple of threads and stuck. split pin broken found in sump. \n initial few threads of castle nut and shaft was found flattened. The shaft alignment was discovered to be normal.\n","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","AE #1 attached lube oil pump shaft key fabricated. AE#1 attached LO pump dismantled, bearings removed. LO pump gear key area filed and made ready. LO pump gear polished and made ready for assembly. Key tried out on the new shaft , found satisfactory.","2022-10-08T08:00:00","","Completed","2022-10-06T08:00:00","No","No","No","Internal"]
[null,null,null,null,54980,"93_Sun Oct 16 2022 04:45:48 GMT+0800","2022-10-06T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Incinerator D.O. burner found misfiring","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","Upon inspection found that one of the ignition cable burnt out. Renewed the ignition cable and layed out a new thermal resistant sleeve on the cable and spark test checked from the test panel. All found to be in good order.  ","2022-10-10T08:00:00","","Completed","2022-10-06T08:00:00","No","No","No","Internal"]
[null,null,null,null,34751,"93_Sun Oct 16 2022 04:47:39 GMT+0800","2022-10-08T08:00:00","Observation","Ship Staff","Ship Staff Insp.","AE#3 exhaust side found leaking with exhaust gas.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Exhaust manifold insulation removed, checked the exact location of leaking. Found leak from exhaust pipe connecting cylinder head gasket. Gasket removed and new gasket placed. AE tried out, working satisfactory without any exhaust gas leak. Insulation fitted back.","2022-10-10T08:00:00","","Completed","2022-10-08T08:00:00","No","No","No","Internal"]
[null,null,null,null,95328,"93_Fri Jul 15 2022 22:21:18 GMT+0800","2022-07-11T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Duct keel mushroom machinal vent top plate thinned down & Hole at Cross deck between Cargo hold no 8 & 9. ","Deck - Pipe / Fittings","General Appearance","External Factors","","","","","Duct keel mushroom machinal vent top plate thinned down area cropped & renewed.","2022-10-10T08:00:00","","Completed","2022-10-01T08:00:00","No","No","No","Internal"]
[null,null,null,null,84671,"93_Sun Oct 16 2022 07:00:04 GMT+0800","2022-10-03T08:00:00","Observation","Ship Staff","Ship Staff Insp.","Wasted monkey island drain pipe (P and S) on bridge wing deck","Accommodation","Structural Condn. / WT integrity ","Equipment Related","","","","","Wasted monkey island drain pipe section cropped and fabricated new section and welded.","2023-01-02T08:00:00","","Completed","2022-10-14T08:00:00","No","No","No","Internal"]
[null,null,null,null,34539,"93_Sun Oct 16 2022 07:45:43 GMT+0800","2022-10-05T08:00:00","Observation","Ship Staff","Ship Staff Insp.","Thinned down and holed Main fire line Between CH No. 4 & 5","Deck - Pipe / Fittings","Safety / LSA / FFA","Equipment Related","","","","","Renewed thinned down and holed section of main fire line on main deck. ","2022-10-12T08:00:00","","Completed","2022-10-08T08:00:00","No","No","No","Internal"]
[null,null,null,null,85216,"93_Sun Oct 16 2022 07:56:30 GMT+0800","2022-10-06T08:00:00","Observation","Ship Staff","Ship Staff Insp.","Heavily rusted and thinned down Hydraulic return line section aft of CH No.8 ","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","","","","","Renewed section of rusted and thinned down hydraulic return line section aft of CH No.8","2022-12-05T08:00:00","","Completed","2022-10-08T08:00:00","No","No","No","Internal"]
[null,null,null,null,98090,"93_Thu Oct 20 2022 22:07:26 GMT+0800","2022-10-20T08:00:00","Breakdown","Ship Staff","Ship Staff Insp.","Cargo hold no.6 hatch cover hydraulic line heavily rusted and thinned down.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","replaced the rusted section of hydraulic pipes for cargo hold no.6","2022-12-31T08:00:00","","Completed","2022-10-20T08:00:00","No","No","No","Internal"]
[null,null,null,null,83663,"93_Sat Oct 29 2022 23:56:21 GMT+0800","2022-10-29T08:00:00","Defect,Observation","Ship Staff","Ship Staff Insp.","Garbage compactor reported not working. ","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","Upon inspection, found that there is no power supply on the compactor. On further inspection, found that the plug was worn out due to ageing. Renewed the same and tried out. system working satisfactory. ","2022-10-31T08:00:00","","Completed","2022-10-29T08:00:00","No","No","No","Internal"]
[null,null,null,null,83248,"93_Tue Nov 15 2022 21:40:37 GMT+0800","2022-11-04T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Fresh water generator high salinity alarm raised. Upon inspection, found ejector pump not creating discharge pressure. ","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","","","","","Checked the ejector pump by removing the cover found that coupling spacer is not rotating after running the motor. Same spacer removed after lifting the motor. Spacer key between the pump coupling and motor coupling adjusted as per maker's instruction manual and fixed back. Ejector pump tried out, found working satisfactory with normal discharge pressure and drawing normal running current. \n","2023-02-03T08:00:00","","Completed","2022-11-04T08:00:00","No","No","No","Internal"]
[null,null,null,null,10486,"93_Tue Nov 15 2022 21:58:25 GMT+0800","2022-11-01T08:00:00","Observation","Ship Staff","Ship Staff Insp.","Sludge shore discharge connection pipeline on stbd side found leaking.","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","External Factors","","","","","Upon inspection found that there was a hole in the pipeline. New pipeline fabricated of same dimension.  After getting office concurrence for hot work , line drained and blanked. Keeping all the safety precautions, fabricated pipeline fitted on the place. Pipeline pressure tested, found no leakages,satisfactory.","2023-01-31T08:00:00","","Completed","2022-11-05T08:00:00","No","No","No","Internal"]
[null,null,null,null,13453,"93_Tue Nov 15 2022 22:05:48 GMT+0800","2022-11-07T08:00:00","Observation,Defect","Ship Staff","Ship Staff Insp."," Emergency Fire Pump found tripped. ","Elect. Mach. & Equip.","Emgcy. Systems","Equipment Related","","","","","Upon inspection, found that the start push button from bridge console and the latching block in the local control panel malfunctioning. Renewed the same and tried out. Monitored the parameters. Found working satisfactory. \n","2022-11-09T08:00:00","","Completed","2022-11-07T08:00:00","No","No","No","Internal"]
[null,null,null,null,14068,"93_Tue Nov 15 2022 22:17:36 GMT+0800","2022-11-09T08:00:00","Defect,Observation","Ship Staff","Ship Staff Insp.","1. Incinerator found misfiring. ","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","Burner unit removed and blanked. Upon inspection, found that the electrode cables are burnt out. Rubber insulation tape wrapped up and thermal resistant sleeve put on the cables. Spark test carried out from the test panel. Burner fixed back and tried out. System working satisfactory. \n","2022-11-12T08:00:00","","Completed","2022-11-09T08:00:00","No","No","No","Internal"]
[null,null,null,null,31645,"93_Sun Nov 20 2022 21:02:40 GMT+0800","2022-11-10T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Fire line leaks observed during pressure test.","LSA / FFA","Emgcy. Systems","Equipment Related","","","","","Leaks marked on fire line , hot work permit requested from office , leaking section of the fire line replaced with sleeves at both ends of inserted section.","2023-01-09T08:00:00","","Completed","2022-11-12T08:00:00","No","No","No","Internal"]
[null,null,null,null,28497,"93_Sun Nov 20 2022 21:14:27 GMT+0800","2022-11-18T08:00:00","Defect","Ship Staff","Ship Staff Insp.","During inspection found few ballast vents head with flame screen missing / damaged","Hull & Tanks","Cargo / Ballast Systems","Equipment Related","","","","","All ballast vent heads checked and flame screen replaced ","2023-01-19T08:00:00","","Completed","2022-11-19T08:00:00","No","No","No","Internal"]
[null,null,null,null,99147,"0_Fri Jan 27 2023 11:55:54 GMT+0800","2023-01-25T08:00:00","Observation","Ship Staff","Suptd. Insp.","Port and stbd side bunker hose davit slewing bearing to\nbe greased regularly.","Deck - Machinery","General Appearance","Equipment Related","","","","","Port and Stbd bunker davit slewing bearing greased during dry dock, and will continue as per PMS","2023-03-21T08:00:00","","Completed",null,"No","No","No","Internal"]
[null,null,null,null,65779,"93_Sun Oct 30 2022 00:12:44 GMT+0800","2022-10-24T08:00:00","Observation","Ship Staff","Ship Staff Insp.","Forward mast flood lighting in poor condition.  ","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","Upon inspection, found that the casing is in poor condition and the casing is brittle. Reqisition raised for the same. RO no. MOJO220213","2022-12-30T08:00:00","","Completed","2022-12-01T08:00:00","No","No","No","Internal"]
[null,null,null,null,41946,"93_Wed Aug 31 2022 17:08:03 GMT+0800","2022-08-29T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Galley cooking range hot plate breaker found tripped","Elect. Mach. & Equip.","Crew Management","Equipment Related","","","","","heat switch received and replaced. All four hot plates are fully functional. ","2022-10-15T08:00:00","","Completed","2022-12-05T08:00:00","No","No","No","Internal"]
[null,null,null,null,66280,"93_Sun Oct 30 2022 00:09:48 GMT+0800","2022-10-27T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Provision refrigerating compressor abnormal alarm activated. ","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","Upon inspection, found that the main magnetic contactor and auxiliary contactor malfunctioning. Renewed the auxiliary contactor. Vessel does not have spare for Main Magnetic contactor. Requisition raised for the same. RO no. MOJO220210 . Main magnetic contactor replaced from the spares received.  System working satisfactory.","2022-12-20T08:00:00","","Completed","2022-12-01T08:00:00","No","No","No","Internal"]
[null,null,null,null,31430,"93_Fri Sep 30 2022 17:06:21 GMT+0800","2022-09-16T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Main engine #4 unit exhaust gas outlet temperature gave out erratic reading.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Upon inspection, found that the sensor is faulty. Requisition raised for the same with the RO no. MOJO220179 . Spares received and replaced. Found working satisfactory.  ","2022-12-10T08:00:00","","Completed","2022-12-03T08:00:00","No","No","No","Internal"]
[null,null,null,null,52656,"93_Wed Aug 31 2022 16:53:59 GMT+0800","2022-08-19T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Bilge, fire & G.S. pump motor no 1  found tripping.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","Upon inspection, found that the magnetic contactor of was burnt out. cannot reuse.Vessel currently have ROB null. for  Bilge, fire & G.S. pump motor no 1 magnetic contactor  RO has been raised for the same. request no. MOJO220166,currently Bilge, fire & G.S. pump motor no 2 pump is in use.  Spares received and replaced. System working satisfactory. ","2022-12-10T08:00:00","","Completed","2022-12-01T08:00:00","No","No","No","Internal"]
[null,null,null,null,68927,"0_Wed Jan 11 2023 11:45:50 GMT+0800","2023-01-01T08:00:00","Defect","Ship Staff","Ship Staff Insp.","NATURAL VENTS FOR CARGO HOLDS FOUND IN BAD CONDITION SAME TO BE RENEWED","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","VENT FRAMING REMOVED . SAME WAS RENEWED AND FIXED BACK ","2023-02-28T08:00:00","","Completed","2023-01-20T08:00:00","No","No","No","Internal"]
[null,null,null,null,94056,"93_Sun Oct 30 2022 00:52:45 GMT+0800","2022-10-24T08:00:00","Breakdown,Observation","Ship Staff","Ship Staff Insp.","Aux. engine #3 , unit no.3 fuel cam has shifted from place radially by 90 degrees.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","AE#3 ,camshaft renewed with new in dry dock by service technician.\nperformance satisfactory.","2023-01-23T08:00:00","","Completed","2023-01-15T08:00:00","No","No","No","Internal"]
[null,null,null,21893,null,"93_28/9/2021 3:40:48 PM","2022-03-17T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Elevator wire last renewal date is not within last 05 yrs and wire to be renewed.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","Spare wire received at Singapore on 17.10.2021, To be renewed by shore technician at suitable port. DD defct list created for the wire renewal job.\nwire renewed at drydock .","2023-01-31T08:00:00","","Completed","2023-01-14T08:00:00","No","No","No","Internal","Vsl to defer job till DD & to raise DD specs. Specs to be sent to office for review."]
[null,null,null,null,99722,"93_Sun Oct 30 2022 00:46:15 GMT+0800","2022-10-29T08:00:00","Observation,Breakdown","Ship Staff","Ship Staff Insp.","During inspection the attached A/E # 1-Lub. oil pump gear teeth and drive gear teeth found thinned down. A thorough inspection carried out, we found the L.O. pump gear thinned down and teeth profile changed. The Aux. machinery#1- drive gear  teeth found broken (2 no.s).","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Aux machinery drive gear was replaced with new by service technician.\nAttached lub oil pump replaced with overhauled pump.Performance\nsatisfactory ","2023-01-28T08:00:00","","Completed","2023-01-17T08:00:00","No","No","No","Internal"]
[null,null,null,null,46132,"93_Fri Jan 27 2023 16:32:07 GMT+0800","2023-01-27T08:00:00","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Engine room one LO tank level gauge bottom self- closing cock was locked at open position.","Hull & Tanks","Eng. / Strg. Comp.","Human Error","","","","","Locking device removed.  ","2023-01-27T08:00:00","","Completed","2023-01-27T08:00:00","No","No","No","Internal"]
[null,null,null,21897,null,"93_02/10/2021 09:42:38","2021-12-20T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Bunker davit (Port) hoisting and slewing movements are seized.","Deck - Mooring Machinery","Structural Condn. / WT integrity ","Equipment Related","","","","","1. slewing movement made operational by dismantling the davit body and Renewed slewing  bearing and limit switch check and working.","2023-01-31T08:00:00","","Completed","2023-01-10T08:00:00","No","No","No","Internal","completed at DD"]
[null,null,null,24609,null,"93_01/02/2022 09:31:31","2021-12-23T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Ch No.2 Bilge Pipe stbd side  damged around 4 mtrs at a height of 8 t0 10 mtrs above the tank top.","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","Equipment Related","","","","","Full section of pipe in cargo hold was renewed at dry dock","2023-01-31T08:00:00","","Completed","2023-01-11T08:00:00","No","No","No","Internal","Job will be attended during DD.,"]
[null,null,null,24610,null,"93_01/02/2022 09:41:08","2021-12-23T08:00:00","Defect","Ship Staff","Ship Staff Insp.","WBT No. 5 stbd side indicator  guage pipe going through the C h No.9 leaking  from the height about 13-14 mtrs above the tank top.","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","Equipment Related","","","","","Full section of pipe inside cargo hold was renewed.","2023-01-31T08:00:00","","Completed","2023-01-13T08:00:00","No","No","No","Internal","Job will be carried out during DD"]
[null,null,null,24611,null,"93_01/02/2022 09:47:24","2021-12-25T08:00:00","Defect","Ship Staff","Ship Staff Insp.","WBT No.3 port side indicator guage pipe passing through the Ch NO.6 is leaking from the upper end of the cargo hold.","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","Equipment Related","","","","","Full section of pipe inside cargo hold was renewed.","2023-01-31T08:00:00","","Completed","2023-01-13T08:00:00","No","No","No","Internal","Job will be attended during DD."]
[null,null,null,24607,null,"93_16/2/2022 3:00:39 AM","2022-02-12T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Cargo Hold Bilge Pipes for  Ch No.2(P),Ch No.3(P),Ch No.4(P),Ch No.6(P&S),CH NO.7 (P),Ch no.8(P)are severly corroded,wasted and have holed.","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","Equipment Related","","","","","Full section of pipes inside cargo hold was renewed.","2022-08-31T08:00:00","SDR 1 DK 11","Completed","2023-01-13T08:00:00","Yes","No","No","Internal","Jobs will be attended during DD>"]
[null,null,null,23031,null,"93_15/11/2021 11:42:35 PM","2022-03-07T08:00:00","Defect","Ship Staff","Ship Staff Insp.","In Ballast control room, Gauges for Ballast tanks No. 3 (P), 4 (P,S), 5 (S) CH-6 and APT are inoperational.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","","","","","At dry dock service engr attended the vessel and all guages were checked and now all are working properly except APT","2023-01-31T08:00:00","","Completed","2023-01-13T08:00:00","No","No","No","Internal","Job to be carried out in upcoming DD."]
[null,null,null,null,56544,"93_Sun May 01 2022 16:03:58 GMT+0800","2022-04-30T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Water leakage in cargo holds no 2, 6, 8, 9 from gauge pipe of WBT No 1P, 3P, 4P, 5P. Gauge pipes of all WBT passing through cargo holds are in bad condition.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","","","","","Full section of pipes inside cargo holds was renewed.","2023-01-31T08:00:00","","Completed","2023-01-13T08:00:00","No","No","No","Internal","Job will be carried out in DD."]
[null,null,null,null,28646,"0_Wed Jan 11 2023 11:41:33 GMT+0800","2023-01-01T08:00:00","Defect","Ship Staff","Ship Staff Insp.","BALLAST CONTROL PANEL SOME INDICATORS ARE NOT WORKING CORRECTLY","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","SERVICE ENGR ATTENDED AT DRY DOCK NOW ALL INDICATION WORKING PROPERLY","2023-02-28T08:00:00","","Completed","2023-01-14T08:00:00","No","No","No","Internal"]
[null,null,null,null,66102,"93_Wed Jan 11 2023 12:20:37 GMT+0800","2023-01-01T08:00:00","Defect","Ship Staff","Ship Staff Insp.","INDICATORS FOR DUCK KEEL FAN , EMERGENCY FIRE PUMP NOT WORKING AND BUZZER SOUND FOR VARIOUS INDICATORS ON THE BRIDGE CONSOLE NOT WORKING.","Deck - Machinery","Emgcy. Systems","Equipment Related","","","","","Renewed the lamps and tried out.  lamps get fused as soon as we start emergency fire pump. Checked the diode circuit for the lamp, found 2 of the 10 diodes in the card are defective. Even with the diode circuit disconnected, same issue exists. AWAITING SERVICE ENGINEER TO INSPECT THE CONTROL SYSTEM. Awaiting spare for Buzzer sound unit to rectify (RO Raised -  MOJO230001)","2023-02-28T08:00:00","","Completed","2023-01-20T08:00:00","No","No","No","Internal"]
[null,null,null,null,95369,"93_Wed Jan 11 2023 11:34:32 GMT+0800","2023-01-11T08:00:00","Defect","Ship Staff","Ship Staff Insp.","AFT WISTLE ON MAIN MAST NOT WORKING","Navigation - GMDSS & Communication","Navigation","Equipment Related","","","","","awaiting service engineer attendance. Rectified  and tried out. System working satisfactory.","2023-02-28T08:00:00","","Completed","2023-01-22T08:00:00","No","No","No","Internal"]
[null,null,null,null,52603,"93_Fri Sep 30 2022 17:15:18 GMT+0800","2022-09-22T08:00:00","Defect","Ship Staff","Ship Staff Insp.","No light indication in hypermist local fire fighting alarm panel on bridge. ","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","Checked the condition of the bulbs, found to be in good condition. Checked  the continuity of the fuses and found to be good. Further inspected the dimmer switch which is connected to the lamp circuit and found defective.  rectified the same. ","2022-12-20T08:00:00","","Completed","2022-12-08T08:00:00","No","No","No","Internal"]
[null,null,null,null,90463,"0_Fri Jan 27 2023 11:52:47 GMT+0800","2023-01-26T08:00:00","Observation","Ship Staff","Suptd. Insp.","Newly fabricated hydraulic pipe to be inspected regularly,\nkeep monitoring, to avoid rust development.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","","","","","two coats of primer applied and final coat in progress","2023-02-25T08:00:00","","Completed","2023-02-06T08:00:00","No","No","No","Internal"]
[null,null,null,null,83443,"0_Fri Jan 27 2023 12:05:11 GMT+0800","2023-01-26T08:00:00","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Laundry room to be cleaned","Accommodation","General Appearance","Behaviour Based","","","","","Laundry room to be cleaned and maintained properly","2023-01-31T08:00:00","","Completed","2023-02-05T08:00:00","No","No","No","Internal"]
[null,null,null,null,65395,"0_Fri Jan 27 2023 12:06:06 GMT+0800","2023-01-27T08:00:00","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","All public toilet to be cleaned and keep tidy.","Accommodation","General Appearance","Behaviour Based","","","","","All public toilet to be cleaned and kept tidy ","2023-01-31T08:00:00","","Completed","2023-02-05T08:00:00","No","No","No","Internal"]
[null,null,null,null,47224,"0_Fri Jan 27 2023 12:04:06 GMT+0800","2023-01-26T08:00:00","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Engine and Deck changing room to be cleaned , keep tidy.","Accommodation","General Appearance","Behaviour Based","","","","","Engine and Deck changing room to be properly cleaned and maintained","2023-01-31T08:00:00","","Completed","2023-02-03T08:00:00","No","No","No","Internal"]
[null,null,null,null,89139,"0_Fri Jan 27 2023 11:45:59 GMT+0800","2023-01-26T08:00:00","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Port and stbd side bunker hose davit to be de-rusted and\ncoated","Deck - Machinery","General Appearance","Equipment Related","","","","","Port and STBD bunker hose davit de-rusted and painted at singapore anchorage","2023-03-26T08:00:00","","Completed","2023-02-08T08:00:00","No","No","No","Internal"]
[null,null,null,null,96552,"0_Fri Jan 27 2023 12:00:55 GMT+0800","2023-01-26T08:00:00","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","All hatch cover control block to be de-rusted and coated","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","All hatch cover control blocks de-rusted, cleaned of oil and coated.","2023-03-30T08:00:00","","Completed","2023-02-13T08:00:00","No","No","No","Internal"]
[null,null,null,null,51399,"0_Fri Feb 17 2023 16:45:42 GMT+0800","2023-02-16T08:00:00","Non Conformity","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Maindeck, port side pilot ladder bottom rubber step rope\nwas looped without any chokes and seizing rope/clamps.","Miscellaneous","ISM Related","Equipment Related","","","","","New pilot ladder ordered and old ladder replaced with new ladder and photos send to right ship for closure.","2023-02-28T08:00:00","MOJO230047","Completed","2023-02-17T08:00:00","No","No","No","Internal"]
[null,null,null,null,76042,"93_Sat Feb 18 2023 09:04:32 GMT+0800","2023-02-15T08:00:00","Observation","Others (Eg. Insurance etc.)","OM Insp. (Eg. SIRE / CDI etc.)","Engine room gas burning equipment flexible hose tail was secured with adjustable/detachable clamps.","Miscellaneous","Eng. / Strg. Comp.","Knowledge Based","","","","","All adjustable clamp replaced with Ear clamp which is supplied by the office in singapore.","2023-02-20T08:00:00","","Completed","2023-02-17T08:00:00","No","No","No","External"]
[null,null,null,null,20895,"93_Sat Feb 18 2023 09:10:37 GMT+0800","2023-02-15T08:00:00","Observation","Others (Eg. Insurance etc.)","OM Insp. (Eg. SIRE / CDI etc.)","ME fuel oil circulating pump was leaking from the seal. ","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","","","","","Immediately changed the seal before the right ship inspector leaves. ","2023-02-15T08:00:00","","Completed","2023-02-15T08:00:00","No","No","No","External"]
[null,null,null,null,68279,"93_Sat Feb 18 2023 09:16:25 GMT+0800","2023-02-15T08:00:00","Observation","Others (Eg. Insurance etc.)","OM Insp. (Eg. SIRE / CDI etc.)","Engine room overhead longitudinal \"I\" beam was not marked with SWL in place","Miscellaneous","General Appearance","Knowledge Based","","","","","Immediately stenciled the beam with SWL marking. ","2023-02-15T08:00:00","","Completed","2023-02-15T08:00:00","No","No","No","External"]
[null,null,null,null,24328,"93_Sat Feb 18 2023 09:24:16 GMT+0800","2023-02-15T08:00:00","Observation","Others (Eg. Insurance etc.)","OM Insp. (Eg. SIRE / CDI etc.)","The incinerator refractory was observed to damage about 20cm X 20 cm.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","Refractory immediately patched up.","2023-02-15T08:00:00","","Completed","2023-02-15T08:00:00","No","No","No","External"]
[null,null,null,null,65380,"93_Fri Jan 27 2023 18:10:39 GMT+0800","2023-01-27T08:00:00","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Refrigeration compressor to be overhauled and renew defect piston.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Renewal of refrigeration compressor defect piston with spare received.","2023-02-11T08:00:00","","Completed","2023-02-23T08:00:00","No","No","No","Internal"]
[null,null,null,null,65686,"93_Fri Jan 27 2023 16:58:51 GMT+0800","2023-01-27T08:00:00","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Steering gear room oil trip tray to be cleaned thoroughly.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Steering gear trip tray to be oil free ","2023-02-03T08:00:00","","Completed","2023-02-14T08:00:00","No","No","No","Internal"]
[null,null,null,null,97794,"93_Fri Jan 27 2023 16:55:30 GMT+0800","2023-01-27T08:00:00","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","HFO transfer pump suction strainer air purge pipe to fabricate and extended to avoid oil purge tank top directly.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","","","","","Purge pipe to be modified.","2023-02-06T08:00:00","","Completed","2023-02-14T08:00:00","No","No","No","Internal"]
[null,null,null,null,80696,"93_Fri Jan 27 2023 16:35:26 GMT+0800","2023-01-27T08:00:00","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","AE 1,2,3 body to be cleaned properly.","E/R - Aux. Engine","General Appearance","Equipment Related","","","","","AE 1,2,3 body to be cleaned.","2023-02-03T08:00:00","","Completed","2023-02-13T08:00:00","No","No","No","Internal"]
[null,null,null,null,69799,"93_Fri Jan 27 2023 16:39:25 GMT+0800","2023-01-27T08:00:00","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","AE 1,2,3 oil trip tray drain pipe to be clear internally.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Drain line of AE 1,2,3 trip tray to be cleared.","2023-02-03T08:00:00","","Completed","2023-02-13T08:00:00","No","No","No","Internal"]
[null,null,null,null,18265,"93_Tue Feb 28 2023 11:40:35 GMT+0800","2023-02-13T08:00:00","Observation","Ship Staff","Ship Staff Insp.","HFO PURIFIER WAS NOT OPERATIONAL DUE TO MOTOR BURNED","E/R - Purifier","Eng. / Strg. Comp.","Equipment Related","","","","","MOTOR RENEWED AND SOME OPERATIONAL ISSUE WAS THEIR SAME RECTIFIED AT THE SAME TIME.","2023-03-09T08:00:00","","Completed","2023-02-23T08:00:00","No","No","No","Internal"]
[null,null,null,null,10975,"93_Fri Feb 17 2023 16:42:29 GMT+0800","2023-02-16T08:00:00","Non Conformity","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Bridge, vessel manoeuvring information poster was not\ncomplied with IMO resolution A601 (15).Track reach\ninformation was not marked.","Navigation - Others","Navigation","Inappropriate Procedure","","","","","Vessel updated track reach information as instructed by LR Class","2023-04-30T08:00:00","","Completed","2023-02-23T08:00:00","No","No","No","Internal"]
[null,null,null,null,43545,"0_Fri Jan 27 2023 11:42:18 GMT+0800","2023-01-26T08:00:00","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Funnel body to be painted.","Accommodation","General Appearance","Equipment Related","","","","","Funnel structure de-rususting and painting completed","2023-03-30T08:00:00","","Completed","2023-02-25T08:00:00","No","No","No","Internal"]
[null,null,null,null,11614,"93_Fri Jan 27 2023 16:42:14 GMT+0800","2023-01-27T08:00:00","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Main engine body to be cleaned thoroughly.","E/R - Main Engine","General Appearance","Equipment Related","","","","","Main engine body to be cleaned thoroughly.","2023-02-03T08:00:00","","Completed","2023-02-14T08:00:00","No","No","No","Internal"]
[null,null,null,null,70134,"93_Fri Jan 27 2023 16:46:16 GMT+0800","2023-01-27T08:00:00","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Emergency fire pump body to be de-rusted and painted.","E/R - Pumps","Emgcy. Systems","Equipment Related","","","","","Emergency fire pump body rusted portion to be de-rusted and painted.","2023-02-03T08:00:00","","Completed","2023-02-11T08:00:00","No","No","No","Internal"]

{"sheet":"Calc","index":2,"n_rows":28,"n_cols":12,"rows_kept":28,"cut":false,"hidden":true,"merged":[]}
["Def_type","Def_cause","Equipments","VIQrefno","Observer_code"]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,"Dim itemSele As Long"]
[null,null,null,null,null,null,null,null,null,null,null,"   dim startRow as integer"]
[null,null,null,null,null,null,null,null,null,null,null,"   startRow=1"]
[null,null,null,null,null,null,null,null,null,null,null,"        For itemSele = 0 To ListBox1.ListCount - 1"]
[null,null,null,null,null,null,null,null,null,null,null,"        If ListBox1.Selected(itemSele) = True Then"]
[null,null,null,null,null,null,null,null,null,null,null,"        Worksheets(\"WorksheetName\").Range(\"A\" & startRow).Value = ListBox1.List(itemSele)"]
[null,null,null,null,null,null,null,null,null,null,null,"        startRow = startRow + 1"]
[null,null,null,null,null,null,null,null,null,null,null,"        End If"]
[null,null,null,null,null,null,null,null,null,null,null,"        Next"]
[null,null,null,null,null,null,null,null,null,null,null,"Dim LastRowA As String"]
[null,null,null,null,null,null,null,null,null,null,null,"        Dim itemSele As Long"]
[null,null,null,null,null,null,null,null,null,null,null,"       Dim startRow as integer"]
[null,null,null,null,null,null,null,null,null,null,null,"        LastRowA = ActiveSheet.Cells(Rows.count, \"A\").End(xlUp).row"]
[null,null,null,null,null,null,null,null,null,null,null,"        startQue = 0"]
[null,null,null,null,null,null,null,null,null,null,null,"        For itemSele = 0 To ListBox1.ListCount - 1"]
[null,null,null,null,null,null,null,null,null,null,null,"        For startRow = 1 To LastRowA"]
[null,null,null,null,null,null,null,null,null,null,null,"        If Worksheets(\"WorksheetName\").Range(\"A\" & startRow).Value = ListBox1.List(itemSele) Then"]
[null,null,null,null,null,null,null,null,null,null,null,"        ListBox1.Selected(itemSele) = True"]
[null,null,null,null,null,null,null,null,null,null,null,"        Exit For"]
[null,null,null,null,null,null,null,null,null,null,null,"        End If"]
[null,null,null,null,null,null,null,null,null,null,null,"        Next j"]
[null,null,null,null,null,null,null,null,null,null,null,"        Next"]
[null,null,null,null,null,null,null,null,null,null,null,"        End If"]

{"sheet":"Areaofobs","index":3,"n_rows":17,"n_cols":2,"rows_kept":17,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Cargo / Ballast Systems",11]
["Cert. & Docu.",2]
["Communication",6]
["Crew Management",3]
["Emgcy. Systems",13]
["Eng. / Strg. Comp.",14]
["General Appearance",15]
["Ice Opns.",17]
["ISM Related",7]
["ISPS Related",10]
["MARPOL Related",9]
["MLC Related",4]
["Mooring",12]
["Navigation",5]
["Safety / LSA / FFA",8]
["Structural Condn. / WT integrity ",16]

{"sheet":"Vessel_type","index":4,"n_rows":1,"n_cols":2,"rows_kept":1,"cut":false,"hidden":true,"merged":[]}
["Vessel_type","ID"]

{"sheet":"Deficiency_type","index":5,"n_rows":8,"n_cols":3,"rows_kept":8,"cut":false,"hidden":true,"merged":[]}
["TITLE","Type of deficiency_description","ID"]
["Breakdown",null,6]
["Critical Equipment",null,4]
["Defect",null,1]
["Guarantee Claim",null,8]
["Non Conformity",null,2]
["Observation",null,3]
["Other",null,7]

{"sheet":"VIQrefno","index":6,"n_rows":1,"n_cols":3,"rows_kept":1,"cut":false,"hidden":true,"merged":[]}
["VIQ_ref_no","Risk Value of observation","ID"]

{"sheet":"Equipment_list","index":7,"n_rows":28,"n_cols":3,"rows_kept":28,"cut":false,"hidden":true,"merged":[]}
["TITLE","Equipment_list_description","ID"]
["Accommodation",null,12]
["Cargo Mach.",null,13]
["Critical Equip.",null,16]
["Deck - Machinery",null,18]
["Deck - Mooring Machinery",null,15]
["Deck - Pipe / Fittings",null,20]
["Documentation",null,21]
["E/R - Air Comp.",null,8]
["E/R - Aux. Engine",null,4]
["E/R - Aux. Mach.",null,7]
["E/R - Boiler",null,5]
["E/R - Main Engine",null,3]
["E/R - Pipes/ valves & fittings",null,9]
["E/R - Pumps",null,32]
["E/R - Purifier",null,6]
["Elect. Mach. & Equip.",null,10]
["Hull & Tanks",null,19]
["Inert Gas",null,14]
["LSA / FFA",null,17]
["Miscellaneous",null,22]
["Navigation - DGPS / EPFS / AIS",null,28]
["Navigation - ECDIS",null,25]
["Navigation - Echo Sounder / Speed Log",null,26]
["Navigation - GMDSS & Communication",null,23]
["Navigation - Others",null,11]
["Navigation - RADAR",null,24]
["Navigation - VDR / BNWAS",null,30]

{"sheet":"PSC_MOU","index":8,"n_rows":11,"n_cols":3,"rows_kept":11,"cut":false,"hidden":true,"merged":[]}
["TITLE","PSC_MOU_description","ID"]
["Asia and the Pacific",null,2]
["Caribbean",null,4]
["Europe and the North Atlantic",null,1]
["Latin America",null,3]
["The Black Sea region",null,6]
["The Indian Ocean",null,8]
["The Mediterranean",null,7]
["The Riyadh MoU",null,9]
["USCG",null,10]
["West and Central Africa",null,5]

{"sheet":"Inspection_type","index":9,"n_rows":13,"n_cols":2,"rows_kept":13,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Bunkering Audit",14]
["Cargo Audit",17]
["Engineering Audit",16]
["ISM Audit",2]
["ISPS Audit",3]
["IT Audit",10]
["MLC Audit",1]
["Mooring Audit",9]
["Nav Audit / Verification",8]
["Onboard Training",18]
["Ship Staff Insp.",15]
["Suptd. Insp.",13]

{"sheet":"Deficiency_Cause","index":10,"n_rows":8,"n_cols":3,"rows_kept":8,"cut":false,"hidden":true,"merged":[]}
["TITLE","Deficiency_Cause_description","ID"]
["Behaviour Based",null,1]
["Equipment Related",null,4]
["External Factors",null,5]
["Human Error",null,7]
["Inappropriate Procedure",null,8]
["Industry Issue",null,6]
["Knowledge Based",null,3]

{"sheet":"Observer_code","index":11,"n_rows":3,"n_cols":3,"rows_kept":3,"cut":false,"hidden":true,"merged":[]}
["TITLE","Observer_code_description","ID"]
["Owner / Marine / Tech. Suptd.",null,3]
["Ship Staff",null,2]

{"sheet":"Status_code","index":12,"n_rows":6,"n_cols":3,"rows_kept":6,"cut":false,"hidden":true,"merged":[]}
["TITLE","Status_code_description","ID"]
["Completed",null,6]
["Deferred to D D",null,5]
["In progress",null,3]
["Not Started",null,2]
["Waiting spare",null,4]

{"sheet":"PSC_ref_no","index":13,"n_rows":19,"n_cols":2,"rows_kept":19,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Alarms",9]
["Cargo operations including equipment",7]
["Certificates & Documentation",2]
["Dangerous Goods",13]
["Emergency Systems",5]
["Fire safety",8]
["ISM",16]
["ISPS",17]
["Life saving appliances",12]
["MLC, 2006",18]
["Other",19]
["Pollution Prevention",15]
["Propulsion and auxiliary machinery",14]
["Radio communication",6]
["Safety of Navigation",11]
["Structural condition",3]
["Water/Weathertight condition",4]
["Working and Living Conditions",10]

{"sheet":"Risk_value_of_obs","index":14,"n_rows":1,"n_cols":2,"rows_kept":1,"cut":false,"hidden":true,"merged":[]}
["Risk Value of observation","ID"]

{"sheet":"Year","index":15,"n_rows":18,"n_cols":1,"rows_kept":18,"cut":false,"hidden":true,"merged":[]}
["Year"]
[2014]
[2015]
[2016]
[2017]
[2018]
[2019]
[2020]
[2021]
[2022]
[2023]
[2024]
[2025]
[2026]
[2027]
[2028]
[2029]
[2030]

{"sheet":"Month","index":16,"n_rows":13,"n_cols":1,"rows_kept":13,"cut":false,"hidden":true,"merged":[]}
["Month"]
["Jan"]
["Feb"]
["Mar"]
["Apr"]
["May"]
["Jun"]
["Jul"]
["Aug"]
["Sep"]
["Oct"]
["Nov"]
["Dec"]

{"sheet":"Date_","index":17,"n_rows":32,"n_cols":1,"rows_kept":32,"cut":false,"hidden":true,"merged":[]}
["Date"]
["01"]
["02"]
["03"]
["04"]
["05"]
["06"]
["07"]
["08"]
["09"]
[10]
[11]
[12]
[13]
[14]
[15]
[16]
[17]
[18]
[19]
[20]
[21]
[22]
[23]
[24]
[25]
[26]
[27]
[28]
[29]
[30]
[31]

{"sheet":"Sheet1","index":18,"n_rows":24,"n_cols":6,"rows_kept":24,"cut":false,"hidden":true,"merged":[]}
[]
[null,"ID","E",null,"Date Recorded",1]
[null,"UNIQUE ID","F",null,"Type of Deficiency",2]
[1,"Date Recorded","G",null,"Observer code",3]
["ignore","Vessel Type","H",null,"Type of Inspection",4]
[null,"Internal / External","I",null,"Description of Deficiency",5]
[null,"Drydock","J",null,"Equipment Categories",6]
[null,"Information Sharing","K",null,"Area of Observation",7]
[null,"Critical_item","L",null,"Deficiency Cause",8]
[null,"Deficiency Type","M",null,"VIQ Ref Number",9]
[null,"Deficiency Cause","N",null,"Risk Value of Obs",10]
[null,"Inspection Type","O",null,"PSC Ref Number",11]
[null,"Equipments","P",null,"PSC MOU ID",12]
[null,"VIQ Reference Number","Q",null,"Action Taken or Required",13]
[null,"Risk Value of the observation","R",null,"Target Date",14]
[null,"PSC Reference Number","S",null,"PO Ref No.",15]
[null,"PSC MOU","T",null,"Status Code",16]
[null,"Observer Code","U",null,"Date Completed",17]
[null,"Target Date","V",null,"Drydock",18]
[null,"Status Code","W",null,"Info Sharing",19]
[null,"Description of Deficiency","X",null,"Critical Item Flag",20]
[null,"Action taken / required","Y",null,"Audit Type",21]
[null,"PO ref no","Z"]
[null,"Date completed","AA"]

{"sheet":"Ship_information","index":19,"n_rows":2,"n_cols":3,"rows_kept":2,"cut":false,"hidden":true,"merged":[]}
["Ship_ID","Ship_Name","FILE_NAME"]
["93","MOJO (19-05-2022)","93_1652941989197.xlsm"]

{"sheet":"External_Deficiency_type","index":20,"n_rows":5,"n_cols":3,"rows_kept":5,"cut":false,"hidden":true,"merged":[]}
["TITLE","Type of deficiency_description","ID"]
["Condn of Class / Memo",null,5]
["Defect",null,1]
["Non Conformity",null,2]
["Observation",null,3]

{"sheet":"External_Inspection_type","index":21,"n_rows":11,"n_cols":2,"rows_kept":11,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Cargo Audit",17]
["Flag State Insp.",5]
["ISM Audit",2]
["ISPS Audit",3]
["MLC Audit",1]
["Nav Audit / Verification",8]
["OM Insp. (Eg. SIRE / CDI etc.)",6]
["Others (Eg. Insurance etc.)",12]
["PSC Inspection",4]
["Terminal Insp.",11]

{"sheet":"External_Observer_code","index":22,"n_rows":7,"n_cols":3,"rows_kept":7,"cut":false,"hidden":true,"merged":[]}
["TITLE","Observer_code_description","ID"]
["Class Surveyor",null,4]
["FSC Inspector",null,5]
["Others (Eg. Insurance etc.)",null,9]
["PSC Insp.",null,6]
["SIRE / CDI Insp.",null,8]
["Terminal Insp.",null,7]

{"sheet":"Sheet Version","index":23,"n_rows":2,"n_cols":2,"rows_kept":2,"cut":false,"hidden":true,"merged":[]}
["Version","Title"]
["2.0","Version 2.0"]