{"text_format":"1","workbook":"xlsx","n_sheets":24,"sheets":["Mainsheet","Completed","Calc","Areaofobs","Vessel_type","Deficiency_type","VIQrefno","Equipment_list","PSC_MOU","Inspection_type","Deficiency_Cause","Observer_code","Status_code","PSC_ref_no","Risk_value_of_obs","Year","Month","Date_","Sheet1","Ship_information","External_Deficiency_type","External_Inspection_type","External_Observer_code","Sheet Version"],"not_rendered":{"charts":0,"images":1,"macros":1,"external_links":0,"defined_names":12,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Mainsheet","index":0,"n_rows":23,"n_cols":28,"rows_kept":23,"cut":false,"hidden":false,"merged":[[10,8,10,9],[10,12,10,13],[12,6,12,27],[8,6,8,27]]}
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,"Defect - Damage Monitoring Sheet"]
[]
[null,null,null,null,null,null,null,"Date of Report","15-Mar-2023",null,null,"Ship Name","DHT EUROPE (02-12-2022)"]
[]
[null,null,null,null,null,null,"VERSION : 2.0"]
[]
[]
[]
[null,null,null,"ID","SHIPSIDE UNIQUEID","UNIQUE ID","Date Recorded","Type of Deficiency","Observer code","Type of Inspection","Description of Deficiency","Equipment Categories","Area of Observation","Deficiency Cause","VIQ Ref Number","Risk Value of Obs","PSC Ref Number","PSC MOU ID","Action Taken or Required","Target Date","PO Ref No.","Status Code","Date Completed","Drydock","Info Sharing","Critical Item","Audit Type","Superintendent Remarks"]
[null,null,null,null,16354,"88_Wed Nov 16 2022 15:01:15 GMT+0800","2022-11-11T08:00:00","Defect","Ship Staff","Ship Staff Insp.","BWTS TRO drain tank discharge pump in pump room not working.","Miscellaneous","Cargo / Ballast Systems","Equipment Related","6.21","High","","","Requisition # DEUR230044 raised. Pump to be replaced once received.","2023-03-31T08:00:00","DEUR230044","Waiting spare",null,"No","No","No","Internal"]
[null,null,null,null,90813,"88_Tue Jan 17 2023 15:55:32 GMT+0800","2023-01-15T08:00:00","Observation,Breakdown","Ship Staff","Ship Staff Insp.","Cargo line 2P Manifold pressure transmitter showing erratic  -ve reading.  Opened and found all connections intact. Suspect diaphragm malfunction.","Navigation - DGPS / EPFS / AIS,Cargo Mach.","Cargo / Ballast Systems","Equipment Related","6.4","High","","","Requisition raised. ","2023-03-31T08:00:00","DEUR230046","Waiting spare",null,"No","No","No","Internal"]
[null,null,null,null,96741,"88_Thu Mar 02 2023 20:39:09 GMT+0800","2023-02-17T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Hot well salinometer: During discharge operations showing 8.8 ppm on boiler panel, but after securing the plant showing 101.4 ppm","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Checks being carried out as per maker's advise. \nLast msg dated 02/ Mar/2023 to be replied after cargo discharge operations.","2023-03-30T08:00:00","","In progress",null,"No","No","No","Internal"]
[null,null,null,null,97096,"88_Thu Mar 02 2023 20:50:14 GMT+0800","2023-01-28T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Bridge wing stbd ME telegraph: RCS not ready & system failure indication when taking ME controls to bridge wing stbd.","Miscellaneous","Navigation","Equipment Related","4.1","High","","","Office advised to carry out certain checks as per msg dated 01/mar/2023. Same will be checked after departure discharge port.","2023-03-31T08:00:00","","In progress",null,"No","No","No","Internal"]
[null,null,null,null,27942,"88_Thu Mar 02 2023 21:00:04 GMT+0800","2023-02-23T08:00:00","Observation","Ship Staff","Ship Staff Insp.","Mooring winch M$ : hyd oil leak from operating lever","Deck - Mooring Machinery","Mooring","Equipment Related","9.1","Low","","","Leak is very minute. Req # DEUR230052 made. Awaiting spares.","2023-03-31T08:00:00","DEUR230052","Waiting spare",null,"No","No","No","Internal"]
[null,null,null,null,25294,"88_Fri Mar 03 2023 16:54:54 GMT+0800","2023-03-01T08:00:00","Critical Equipment","Ship Staff","Ship Staff Insp.","UV flame detector: body observed cracked and brittle.","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.1","Very High","","","Requisition # DEUR230064 raised.","2023-03-30T08:00:00","","Waiting spare",null,"No","No","No","Internal"]

{"sheet":"Completed","index":1,"n_rows":394,"n_cols":28,"rows_kept":394,"cut":false,"hidden":false,"merged":[[10,8,10,9],[10,12,10,13],[12,6,12,27],[8,6,8,27]]}
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,"Defect - Damage Monitoring Sheet"]
[]
[null,null,null,null,null,null,null,"Date of Report","15-Mar-2023",null,null,"Ship Name","DHT EUROPE (02-12-2022)"]
[]
[null,null,null,null,null,null,"VERSION : 2.0"]
[]
[]
[]
[null,null,null,"ID","SHIPSIDE UNIQUEID","UNIQUE ID","Date Recorded","Type of Deficiency","Observer code","Type of Inspection","Description of Deficiency","Equipment Categories","Area of Observation","Deficiency Cause","VIQ Ref Number","Risk Value of Obs","PSC Ref Number","PSC MOU ID","Action Taken or Required","Target Date","PO Ref No.","Status Code","Date Completed","Drydock","Info Sharing","Critical Item","Audit Type","Superintendent Remarks"]
[null,null,null,9546,null,"88_10/1/2020 5:19:20 AM","2018-12-29T23:59:17","Observation","Ship Staff","Ship Staff Insp.","Walkway areas not clearly marked on port side main deck.","Miscellaneous","General Appearance","Inappropriate Procedure","11.3","Medium","","","Chipping of areas carried out. Painting of all areas carried out with anti skid. Marking of boundaries in progress.","2020-01-26T23:59:17","","Completed","2020-01-21T23:59:17","No","No","No","Internal"]
[null,null,null,2289,null,"88_18/10/2019 2:31:43 AM","2019-08-18T23:59:17","Defect","Ship Staff","Ship Staff Insp.","ME lub oil auto back wash filter Hydraulic motor indicator broken ","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","New hydraulic motor to be replaced","2019-12-10T23:59:17","","Completed","2019-09-13T23:59:17","No","No","No","Internal"]
[null,null,null,2262,null,"88_17/10/2019 10:40:45 AM","2019-08-19T23:59:17","Defect","Ship Staff","Ship Staff Insp.","Hydroblaster inoperational due to lack of spares","Elect. Mach. & Equip.","General Appearance","Equipment Related","","","","","Overhauling carried out, Working satisfactory.","2019-11-15T23:59:17","DEUR195022","Completed","2019-11-06T23:59:17","No","No","No","Internal"]
[null,null,null,2285,null,"88_17/10/2019 1:32:04 PM","2019-08-19T23:59:17","Defect","Ship Staff","Ship Staff Insp.","Hydraulic oil leak on the mooring winch M5 - A small diameter pipe on the return line of mooring winch motor sheared off ","Deck - Machinery,Deck - Pipe / Fittings","Mooring","Equipment Related","9.14","Medium","","","Pipe repaired and Pressure test","2019-08-28T23:59:17","","Completed","2019-08-21T23:59:17","No","No","No","Internal"]
[null,null,null,2286,null,"88_18/10/2019 1:56:57 AM","2019-08-19T23:59:17","Defect","Ship Staff","Ship Staff Insp.","Slight hydraulic oil leak from the control lever of M3 mooring winch, vessel staff changed O rings but leak is persistent. Further investigation required. ","Deck - Pipe / Fittings","Mooring","Equipment Related","9.14","Medium","","","O ring renewed and spol piecce cleaned.Leak rectified.","2019-09-15T23:59:17","","Completed","2019-10-02T23:59:17","No","No","No","Internal"]
[null,null,null,2287,null,"88_18/10/2019 2:22:13 AM","2019-08-19T23:59:17","Defect","Ship Staff","Ship Staff Insp.","BMT Hull stress monitor is not working. As per ship staff the CPU of the unit which is kept on bridge got damaged. ","Deck - Machinery","Cargo / Ballast Systems","Equipment Related","","","","","As discussed with Office same job deffered to DD","2019-08-31T23:59:17","","Completed","2019-09-25T23:59:17","No","No","No","Internal"]
[null,null,null,2288,null,"88_18/10/2019 2:25:24 AM","2019-08-19T23:59:17","Defect","Ship Staff","Ship Staff Insp.","CCTV cameras are inoperational ","Miscellaneous","Communication","Equipment Related","","","","","RO raised by office, CCTVs shall be supplied in Singapore, ship staff to install upon receiving the same","2019-08-31T23:59:17","","Completed","2019-09-25T23:59:17","No","No","No","Internal"]
[null,null,null,2294,null,"88_18/10/2019 3:06:21 AM","2019-08-19T23:59:17","Defect","Ship Staff","Ship Staff Insp.","2 Foam monitors found leaking","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.35","Medium","","","Foam monitor valves repaired","2019-09-05T23:59:17","","Completed","2019-09-05T23:59:17","No","No","No","Internal"]
[null,null,null,2295,null,"88_18/10/2019 3:21:54 AM","2019-08-19T23:59:17","Defect","Ship Staff","Ship Staff Insp.","4 Fire hydrant valves found leaking    ","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.35","Medium","","","Fire hydrants removed, lapping carried out and fitted back","2019-09-05T23:59:17","","Completed","2019-09-05T23:59:17","No","No","No","Internal"]
[null,null,null,2297,null,"88_18/10/2019 3:32:51 AM","2019-08-19T23:59:17","Defect","Ship Staff","Ship Staff Insp.","Slight oil leak observed from STBD windlass hydaulic line flange near deck penetration. ","Deck - Machinery","Mooring","Equipment Related","9.2","Very High","","","Renew / Replace O ring","2019-09-15T23:59:17","","Completed","2019-09-06T23:59:17","No","No","No","Internal"]
[null,null,null,2265,null,"88_17/10/2019 3:19:56 PM","2019-08-23T23:59:17","Defect","Ship Staff","Ship Staff Insp.","PORT LT Cooler, Sea water outlet distance piece/corrosion flange having a minor leak.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Sacrificial flange  renewed","2019-12-25T23:59:17","","Completed","2019-11-02T23:59:17","No","No","No","Internal"]
[null,null,null,2266,null,"88_17/10/2019 3:25:09 PM","2019-08-28T23:59:17","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Bridge telegraph printer not working properly","Navigation - Others","Navigation","Equipment Related","4.7","High","","","On board Repairs caried out.presently working satisfactory","2019-10-15T23:59:17","","Completed","2019-10-13T23:59:17","No","No","No","Internal"]
[null,null,null,5622,null,"88_25/10/2019 6:42:51 AM","2019-08-28T23:59:17","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Water cooler outside ECR, compressor not working","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","New water fountain installed","2019-11-25T23:59:17","DEUR190045","Completed","2019-11-02T23:59:17","No","No","No","Internal"]
[null,null,null,2305,null,"88_17/10/2019 4:12:09 PM","2019-08-29T23:59:17","Defect","Ship Staff","Ship Staff Insp.","Cooling water expansion tank level gauge leaking while checking level","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Leak to be arrested","2019-10-10T23:59:17","","Completed","2019-10-07T23:59:17","No","No","No","Internal"]
[null,null,null,2274,null,"88_17/10/2019 4:38:05 PM","2019-08-29T23:59:17","Defect","Ship Staff","Ship Staff Insp.","Echo Sounder Repeater Screen on Bridge Front Panel Not Visible","Navigation - Echo Sounder / Speed Log","Navigation","Equipment Related","4.7","High","","","New repeater installed","2019-12-25T23:59:17","DEUR190053","Completed","2019-12-21T23:59:17","No","No","No","Internal"]
[null,null,null,2296,null,"88_18/10/2019 3:30:28 AM","2019-08-29T23:59:17","Defect","Ship Staff","Ship Staff Insp.","Paint store sprinkler system valve not holding","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.35","Medium","","","Renew / replace valve","2019-09-08T23:59:17","","Completed","2019-09-07T23:59:17","No","No","No","Internal"]
[null,null,null,2298,null,"88_18/10/2019 3:38:42 AM","2019-08-29T23:59:17","Defect","Ship Staff","Ship Staff Insp.","ME FO auto filter leaking from spindle top","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Seal rings to be renewed","2019-09-25T23:59:17","","Completed","2019-09-10T23:59:17","No","No","No","Internal"]
[null,null,null,2267,null,"88_17/10/2019 3:43:37 PM","2019-08-31T23:59:17","Defect","Ship Staff","Ship Staff Insp.","Pumproom phone communication not audible on Bridge/CCR","Navigation - GMDSS & Communication","Communication","Equipment Related","5.17","Very High","","","Repairs carried out, working satisfactory.","2019-10-15T23:59:17","","Completed","2019-10-07T23:59:17","No","No","No","Internal"]
[null,null,null,2268,null,"88_17/10/2019 3:45:56 PM","2019-08-31T23:59:17","Defect","Ship Staff","Ship Staff Insp.","Foam Hose box Stb side near Manifold poor condition","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.38","High","","","New foam hose box received, same renewed.","2019-10-05T23:59:17","","Completed","2019-10-21T23:59:17","No","No","No","Internal"]
[null,null,null,2290,null,"88_18/10/2019 2:37:13 AM","2019-09-01T23:59:17","Defect","Ship Staff","Ship Staff Insp.","All DGs LO running hours exceed 2000 hrs  ","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","All DGs sump oil renewed","2019-09-10T23:59:17","","Completed","2019-09-07T23:59:17","No","No","No","Internal"]
[null,null,null,2291,null,"88_18/10/2019 2:55:07 AM","2019-09-01T23:59:17","Defect","Ship Staff","Ship Staff Insp.","Both FWGs production very low   ","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Need to check and rectify","2019-09-15T23:59:17","","Completed","2019-09-06T23:59:17","No","No","No","Internal"]
[null,null,null,2293,null,"88_18/10/2019 3:02:52 AM","2019-09-01T23:59:17","Defect","Ship Staff","Ship Staff Insp.","Port life boat engine sound abnormal in AHD direction         ","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.29","High","","","Drive shaft lubricated, noise now normal","2019-09-15T23:59:17","","Completed","2019-09-08T23:59:17","No","No","No","Internal"]
[null,null,null,2299,null,"88_18/10/2019 3:53:36 AM","2019-09-01T23:59:17","Defect","Ship Staff","Ship Staff Insp.","Elevator telephone handset communication not audible","Navigation - GMDSS & Communication","Communication","Equipment Related","","","","","To be repaired","2019-09-25T23:59:17","","Completed","2019-09-19T23:59:17","No","No","No","Internal"]
[null,null,null,2269,null,"88_17/10/2019 4:02:10 PM","2019-09-02T23:59:17","Defect","Ship Staff","Ship Staff Insp.","Light fittings in E/rm cracked same need to be replaced","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","11.1","High","","","WS","2020-01-25T23:59:17","DEUR190037","Completed","2019-12-16T23:59:17","No","No","No","Internal","Target date revised as per vessel request. Job i progress."]
[null,null,null,2302,null,"88_18/10/2019 4:14:48 AM","2019-09-02T23:59:17","Defect","Ship Staff","Ship Staff Insp.","E/r Blower No 2 flap stuck an dnot closing","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.18","High","","","Actuator overhauled flap function normal","2019-09-10T23:59:17","","Completed","2019-09-05T23:59:17","No","No","No","Internal"]
[null,null,null,2300,null,"88_18/10/2019 3:58:32 AM","2019-09-05T23:59:17","Defect","Ship Staff","Ship Staff Insp.","Crew laundry drier not operational","Miscellaneous","General Appearance","Equipment Related","","","","","Drier made operation","2019-09-25T23:59:17","","Completed","2019-09-20T23:59:17","No","No","No","Internal"]
[null,null,null,2301,null,"88_18/10/2019 4:12:42 AM","2019-09-05T23:59:17","Defect","Ship Staff","Ship Staff Insp.","Both LT collers performance bad, may be chocked","Elect. Mach. & Equip.,E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","LT coolers strainer cleaned and chemical circulation carried out","2019-09-15T23:59:17","","Completed","2019-09-14T23:59:17","No","No","No","Internal"]
[null,null,null,2292,null,"88_18/10/2019 2:58:18 AM","2019-09-06T23:59:17","Defect","Ship Staff","Ship Staff Insp.","DG LO purifier temp not coming up     ","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Heater cleaned and control valve overhauled, temp:95","2019-09-15T23:59:17","","Completed","2019-09-09T23:59:17","No","No","No","Internal"]
[null,null,null,2276,null,"88_17/10/2019 4:53:59 PM","2019-09-10T23:59:17","Defect","Ship Staff","Ship Staff Insp.","Bridge Aircon not effective ","E/R - Aux. Mach.","General Appearance","Equipment Related","","","","","Leak arrested","2019-10-25T23:59:17","","Completed","2019-10-22T23:59:17","No","No","No","Internal"]
[null,null,null,2277,null,"88_17/10/2019 5:08:01 PM","2019-09-10T23:59:17","Defect","Ship Staff","Ship Staff Insp.","Steering motor #2 hydraulic lock alarm activating, without effecting the performance ","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Linear synchro needs to be adjusted","2019-10-25T23:59:17","","Completed","2019-10-24T23:59:17","No","No","No","Internal"]
[null,null,null,2275,null,"88_17/10/2019 4:49:58 PM","2019-09-13T23:59:17","Defect","Ship Staff","Ship Staff Insp.","Atmospheric condensor SW outlet pipe holed","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Leak rectified, For permanent repairs vessel needs anchorage","2019-11-25T23:59:17","","Completed","2019-11-28T23:59:17","No","No","No","Internal"]
[null,null,null,2279,null,"88_18/10/2019 1:27:38 AM","2019-09-14T23:59:17","Defect","Ship Staff","Ship Staff Insp.","220 V Insulation low same to be improved","Elect. Mach. & Equip.","Communication","Equipment Related","10.38","Medium","","","Insulation improved to acceptable standards","2020-01-25T23:59:17","","Completed","2019-12-31T23:59:17","No","No","No","Internal","When it is expected to be completed. IT has been so long since the defect is existing."]
[null,null,null,2304,null,"88_18/10/2019 1:48:29 AM","2019-09-25T23:59:17","Defect","Ship Staff","Ship Staff Insp.","Various pressure gauges in E/rm damaged ","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Damaged gauges to be replaced with new ","2019-10-07T23:59:17","","Completed","2019-10-07T23:59:17","No","No","No","Internal"]
[null,null,null,2280,null,"88_18/10/2019 1:46:11 AM","2019-09-25T23:59:17","Defect","Ship Staff","Ship Staff Insp.","Main SW pump pressure transmitter erratic output ","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Transmitter to be checked and calibrated","2019-09-30T23:59:17","","Completed","2019-09-25T23:59:17","No","No","No","Internal"]
[null,null,null,2303,null,"88_18/10/2019 4:19:12 AM","2019-09-25T23:59:17","Defect","Ship Staff","Ship Staff Insp.","Leaking Air line near manifold area","Deck - Pipe / Fittings","General Appearance","Equipment Related","","","","","Repairs to be carried out","2019-09-25T23:59:17","","Completed","2019-09-25T23:59:17","No","No","No","Internal"]
[null,null,null,2281,null,"88_20/10/2019 5:39:16 AM","2019-09-27T23:59:17","Defect","Ship Staff","Ship Staff Insp.","Navtex JRC printer / Printing faded / unreadable","Navigation - GMDSS & Communication","Navigation","Equipment Related","4.7","High","","","New printer received and same renewed.","2019-12-25T23:59:17","","Completed","2019-10-19T23:59:17","No","No","No","Internal"]
[null,null,null,2282,null,"88_20/10/2019 5:42:14 AM","2019-10-06T23:59:17","Defect","Ship Staff","Ship Staff Insp.","VRCS return hydraulic line pin hole leak on deck","Deck - Pipe / Fittings","General Appearance","Equipment Related","","","","","Pipe removed welding carried out and boxed back.","2019-11-25T23:59:17","","Completed","2019-10-16T23:59:17","No","No","No","Internal"]
[null,null,null,2284,null,"88_20/10/2019 5:50:47 AM","2019-10-08T23:59:17","Defect","Ship Staff","Ship Staff Insp.","Aux boiler # 2 Feed water level controller erratic","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Service engineer attended in Fujiarah. System performance shall be tested during discharging operation.","2019-11-05T23:59:17","DEUR195042","Completed","2019-10-28T23:59:17","No","No","No","Internal"]
[null,null,null,5617,null,"88_26/10/2019 9:07:38 AM","2019-10-08T23:59:17","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","FW TANK S VENT HEAD DEFLECTOR PLATE IS CORRODED","Deck - Pipe / Fittings","General Appearance","Equipment Related","","","","","Plate renewed","2019-10-31T23:59:17","","Completed","2019-10-25T23:59:17","No","No","No","Internal"]
[null,null,null,5618,null,"88_25/10/2019 6:46:23 AM","2019-10-08T23:59:17","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Suction and Discharge press gauge of stern tube LO pump no. 2 is not working. To be replaced","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Gauges to be replaced","2019-10-23T23:59:17","","Completed","2019-10-23T23:59:17","No","No","No","Internal"]
[null,null,null,5619,null,"88_25/10/2019 7:14:42 AM","2019-10-08T23:59:17","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","There is an auto bilge water separator installed for incinerator drain, which is not in use any more. Same to be entered in LOTO record book","Documentation","Eng. / Strg. Comp.","Equipment Related","","","","","Entry in LOTO record book","2019-10-23T23:59:17","","Completed","2019-10-19T23:59:17","No","No","No","Internal"]
[null,null,null,5620,null,"88_26/10/2019 8:59:14 AM","2019-10-08T23:59:17","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Spare DG T/C cartridge is store but not covered. The cartridge may get damaged","Miscellaneous","Eng. / Strg. Comp.","Inappropriate Procedure","","","","","To be covered and secured","2019-10-26T23:59:17","","Completed","2019-10-21T23:59:17","No","No","No","Internal"]
[null,null,null,5623,null,"88_25/10/2019 7:02:56 AM","2019-10-08T23:59:17","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Main steam stop valve to COPT near LT coolers, Leaking form the gland. Gland to be tightened or renewed","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Gland to be nipped up / packing to renewed","2019-11-16T23:59:17","","Completed","2019-11-23T23:59:17","No","No","No","Internal"]
[null,null,null,5624,null,"88_25/10/2019 7:16:53 AM","2019-10-08T23:59:17","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Water Cooler on upper deck not operational","Accommodation","MLC Related","Equipment Related","","","","","To  be replace, RO raised","2019-11-16T23:59:17","DEUR190045","Completed","2019-11-23T23:59:17","No","No","No","Internal"]
[null,null,null,5625,null,"88_26/10/2019 9:10:45 AM","2019-10-08T23:59:17","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Spares inventory to be updated in PAL with Loacation","Documentation","Cert. & Docu.","Human Error","","","","","Spares inventory to be updated in PAL with location","2020-01-26T23:59:17","","Completed","2019-12-31T23:59:17","No","No","No","Internal"]
[null,null,null,5626,null,"88_25/10/2019 6:54:17 AM","2019-10-08T23:59:17","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Various save all of bunker tanks capacity plate too rusted to view. Capacity tag plate to cleaned and if required to be stencillled","Miscellaneous","General Appearance","Equipment Related","","","","","Save alls to be de rusted and stencilling to be carried out","2019-10-23T23:59:17","","Completed","2019-10-19T23:59:17","No","No","No","Internal"]
[null,null,null,2306,null,"88_20/10/2019 5:18:18 AM","2019-10-09T23:59:17","Defect","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","Stbd accommodation ladder shifting wire slightly deformed / loose strends","Deck - Machinery","General Appearance","Equipment Related","5.47","Medium","","","Wire renewed with new spare wire onboard","2019-11-15T23:59:17","","Completed","2019-10-13T23:59:17","No","No","No","External"]
[null,null,null,6259,null,"88_19-11-2019 18:46:12","2019-10-09T23:59:17","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Water fountain in upper deck not working","Accommodation","MLC Related","Equipment Related","10.16","Very High","","","Water fountain shall be replaced with new spare","2019-11-10T23:59:17","","Completed","2019-11-23T23:59:17","No","No","No","Internal"]
[null,null,null,2283,null,"88_20/10/2019 5:45:16 AM","2019-10-09T23:59:17","Defect","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","Critical spare part list min requirred showing nil in Pal","Documentation","Cert. & Docu.","Inappropriate Procedure","10.13","Very High","","","Min required spares to be updated in PAL from office","2019-10-09T23:59:17","","Completed","2019-10-13T23:59:17","No","No","No","External"]
[null,null,null,2307,null,"88_20/10/2019 5:22:43 AM","2019-10-13T23:59:17","Defect","Ship Staff","Ship Staff Insp.","Mian Air compr # 1 I stage pressure erratic","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","1st stage suction plate found broken same renewed with new spare","2019-10-15T23:59:17","","Completed","2019-10-13T23:59:17","No","No","No","Internal"]
[null,null,null,2308,null,"88_20/10/2019 5:37:00 AM","2019-10-14T23:59:17","Defect","Ship Staff","Ship Staff Insp.","FWG # 1 vacuum low","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Ejector pump strainer found chocked same cleaned","2019-10-15T23:59:17","","Completed","2019-10-14T23:59:17","No","No","No","Internal"]
[null,null,null,6262,null,"88_19-11-2019 21:45:41","2019-11-02T23:59:17","Defect","Ship Staff","Ship Staff Insp.","Economiser soot blower steam leak from gland","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Leak rectified from gland","2019-12-12T23:59:17","","Completed","2019-12-04T23:59:17","No","No","No","Internal","Does it need complete steam to be shut down to rectify?"]
[null,null,null,6261,null,"88_19-11-2019 18:51:46","2019-11-04T23:59:17","Defect","Ship Staff","Ship Staff Insp.","DG FO auto filter leaking from top cover","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.27","Medium","","","filter top cover O-ring to renewed","2019-12-10T23:59:17","DEUR190008","Completed","2019-12-17T23:59:17","No","No","No","Internal","Will be supplied in Singapore."]
[null,null,null,6266,null,"88_13/11/2019 3:58:37 PM","2019-11-05T23:59:17","Breakdown","Ship Staff","Ship Staff Insp.","FWG#1 Ejector overboard line holed.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.33","High","","","Pipe section removed and new fabricated section fitted","2019-11-10T23:59:17","","Completed","2019-11-06T23:59:17","No","No","No","External"]
[null,null,null,6260,null,"88_19-11-2019 18:48:17","2019-11-06T23:59:17","Defect","Ship Staff","Ship Staff Insp.","ME FO heater #1 steam leak from end cover","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.31","Very High","","","Heater end cover gasket to be renewed","2019-11-27T23:59:17","","Completed","2019-12-01T23:59:17","No","No","No","Internal"]
[null,null,null,6264,null,"88_20-11-2019 14:03:58","2019-11-06T23:59:17","Defect","Ship Staff","Ship Staff Insp.","Jobs to be triggered in PAL","Documentation","ISM Related","Industry Issue","10.29","Medium","","","Jobs triggered in PAL","2019-12-26T23:59:17","","Completed","2019-12-08T23:59:17","No","No","No","Internal","When it is expected to be completed?"]
[null,null,null,6268,null,"88_20-11-2019 14:06:31","2019-11-07T23:59:17","Defect","Ship Staff","Ship Staff Insp.","Sanitary exhaust blower belts loose.","Accommodation","Eng. / Strg. Comp.","Equipment Related","10.15","Low","","","Belts renewed and pulley aligned","2019-11-25T23:59:17","","Completed","2019-11-15T23:59:17","No","No","No","Internal"]
[null,null,null,6267,null,"88_13/11/2019 4:00:56 PM","2019-11-08T23:59:17","Breakdown","Ship Staff","Ship Staff Insp.","ME LO purifier vibration sensor erratic","E/R - Purifier","Eng. / Strg. Comp.","Equipment Related","10.35","Very High","","","Sensor renewed with new spare.","2019-11-10T23:59:17","","Completed","2019-11-08T23:59:17","No","No","No","External"]
[null,null,null,2264,null,"88_17/10/2019 2:05:12 PM","2019-11-19T23:59:17","Defect","Ship Staff","Ship Staff Insp.","ME rpm indicator at local manouvering platform not working.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","defective RPM indicator replaced with spare new one.","2020-02-15T23:59:17","DEUR190044","Completed","2020-02-09T23:59:17","No","No","No","Internal","Spare will be ready by Jan end."]
[null,null,null,2273,null,"88_17/10/2019 4:32:21 PM","2019-11-25T23:59:17","Defect","Ship Staff","Ship Staff Insp.","Sewage holding tank level gauge missing","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Vessel reraised again RO on 3rd March 2020, Vessel received spare level gauge fitted back in holding tank and found working properly.","2020-05-23T23:59:17","DEUR200046","Completed","2020-05-07T23:59:17","No","No","No","Internal","Quote was for 2019 and is cancelled. Please raise RO again."]
[null,null,null,2270,null,"88_17/10/2019 4:06:19 PM","2019-11-28T23:59:17","Defect","Ship Staff","Ship Staff Insp.","ME Bearing wear monitoring system display not operational","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.21","Medium","","","Vessel received Water in Oil sensor while passing Singapore fitted in place working satisfactory.","2020-08-26T23:59:17","DEUR205048","Completed","2020-08-17T23:59:17","No","No","No","Internal","We will supply stand alone water in oil sensor PO no DEUR205048."]
[null,null,null,2271,null,"88_17/10/2019 4:24:01 PM","2019-11-28T23:59:17","Defect","Ship Staff","Ship Staff Insp.","Steering gear #1 and #3 valve block leak from safety valve base","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Leak to be arrested at next available oportunity/ Leak arrested by tightening.","2020-05-23T23:59:17","","Completed","2020-02-27T23:59:17","No","No","No","Internal","Job to be completed at the earliest opportunity or anchorage. Target date revised."]
[null,null,null,8724,null,"88_14/12/2019 10:16:01 AM","2019-11-30T23:59:17","Defect","Ship Staff","Ship Staff Insp.","Cargo and ballast valves noticed to have discrepancy in the indicators. The indicators noticed to sluggish and erratic in some cases","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.11","Medium","","","Vessel renewed  potentiometer received noticed now Valve operating smoothly.","2021-04-10T23:59:17","","Completed","2021-03-20T23:59:17","No","No","No","Internal","Spare supplied to be attended. Target date revised accordingly."]
[null,null,null,8722,null,"88_14/12/2019 10:22:02 AM","2019-12-01T23:59:17","Defect","Ship Staff","Ship Staff Insp.","Hyraulic oil leakgae noticed from actuator of mastriser valve.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","Actuator isolated presently,valve is operational but oil drips from actuator.Leak be rectified by opening the actuator.","2019-12-15T23:59:17","","Completed","2019-12-13T23:59:17","No","No","No","Internal"]
[null,null,null,9547,null,"88_10/01/2020 10:47:19","2019-12-04T23:59:17","Defect","Ship Staff","Ship Staff Insp.","LT cooler SW  flange having small leak","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Valve gasket  renewed","2020-02-23T23:59:17","","Completed","2020-01-22T23:59:17","No","No","No","Internal"]
[null,null,null,8725,null,"88_15/12/2019 7:37:47 AM","2019-12-05T23:59:17","Defect","Ship Staff","Ship Staff Insp.","Soot tank not emptying when ejector is used. Instead level increases suspect overboard valves not opening.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.31","Very High","","","Overboard valves to be renewed","2020-05-05T23:59:17","DEU200048","Completed","2020-03-11T23:59:17","Yes","No","No","Internal","Raise RO for overboad valve."]
[null,null,null,8726,null,"88_18/12/2019 2:54:18 PM","2019-12-06T23:59:17","Defect","Ship Staff","Ship Staff Insp.","ME unit #5 fuel pump inlet valve having small leak","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.31","Very High","","","Valve gasket to be renewed/ Valve flange tightened and observed no leak for last 20 days.","2020-02-23T23:59:17","","Completed","2020-02-24T23:59:17","No","No","No","Internal"]
[null,null,null,8723,null,"88_14/12/2019 10:24:40 AM","2019-12-07T23:59:17","Defect","Ship Staff","Ship Staff Insp.","Hydraulic oil leakage noticed from controller for mooring winch M1. ","Deck - Mooring Machinery","Mooring","Equipment Related","","","","","Controller dismantled. O rings and lip seals renewed and winch tried out. FOund working without any leak.","2019-12-15T23:59:17","","Completed","2019-12-13T23:59:17","No","No","No","Internal"]
[null,null,null,8719,null,"88_22/12/2019 10:55:45 AM","2019-12-11T23:59:17","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Deck locker (S) housekeeping to improve further.","Miscellaneous","General Appearance","Human Error","11.3","Medium","","","Vessel carried out cleaning and arranging of SOPEP locker, deck stores and deck workshop areas. Further painting jobs to be carried out during ballast passage.","2020-02-03T23:59:17","","Completed","2020-01-19T23:59:17","No","No","No","Internal"]
[null,null,null,8720,null,"88_22/12/2019 11:00:33 AM","2019-12-11T23:59:17","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Bosun store davit reported frozen.","Deck - Machinery","General Appearance","Equipment Related","","","","","The davit movable parts seem to have not been greased for a very long time leading to the freezing of the movement. Ol grease pumped out and penetrating oil used. Free movement achieved and greased. Davit rotating freely.","2020-01-10T23:59:17","","Completed","2020-01-01T23:59:17","No","No","No","Internal"]
[null,null,null,8721,null,"88_22/12/2019 11:04:14 AM","2019-12-11T23:59:17","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Windlass (S) claw coupling engaging lever fulcrum pin detached","Deck - Machinery","Mooring","Equipment Related","9.14","Medium","","","Stbd wndlass claw coupling engaging gear dismantled and given to engine room for hotwork in workshop. Unit fitted back in place","2020-03-27T23:59:17","","Completed","2020-01-04T23:59:17","No","No","No","Internal"]
[null,null,null,8727,null,"88_22/12/2019 10:40:47 AM","2019-12-11T23:59:17","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Emergency generator room fixed CO2 fixed installation system release handle door wasted","Deck - Pipe / Fittings","Safety / LSA / FFA","Equipment Related","5.35","Medium","","","The cabinet for CO2 release for emg gen. cabinet reneed with new fabricated box","2020-03-27T23:59:17","","Completed","2020-01-14T23:59:17","No","No","No","Internal"]
[null,null,null,8728,null,"88_22/12/2019 10:43:22 AM","2019-12-11T23:59:17","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Deck workshop entrance step cracked","Accommodation","General Appearance","Equipment Related","11.3","Medium","","","The entrance step renewed by fixing a chequered plate on top of the broken plate by means of cold work.","2020-03-27T23:59:17","","Completed","2020-01-17T23:59:17","Yes","No","No","Internal"]
[null,null,null,8729,null,"88_22/12/2019 10:49:01 AM","2019-12-11T23:59:17","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Main deck walkway chequered plate securing bolts missing.Main deck walkway chequered plate slippery due to thick coat of paint. These plates to be chip & apply thin coat of paint. In case chequered dots are wasted, plate to renew.","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.3","Medium","","","The walkways on deck have wasted areas which ahve been covered with putty and hence the thick coat of paint. The plates to be renewed in dry dock.","2020-03-27T23:59:17","","Completed","2020-03-12T23:59:17","Yes","No","No","Internal"]
[null,null,null,8730,null,"88_22/12/2019 10:52:34 AM","2019-12-11T23:59:17","Defect","Owner / Marine / Tech. Suptd.","Ship Staff Insp.","Cargo tank 1C, 4C, 5C, 3P, 3S & 5P COW machine (1 pc each tank) reported not working","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.34","High","","","Overhauling of all COW machines carried out. Rocker assembly renewed for all damaged ones. Oil and grease renewed for all COW machines. ","2020-05-25T23:59:17","DEUR200065","Completed","2020-05-24T23:59:17","No","No","No","Internal","Has it been tried during this discharging operation?"]
[null,null,null,6263,null,"88_19-11-2019 23:00:37","2019-12-12T23:59:17","Defect","Ship Staff","Ship Staff Insp.","Telephone exchange alarm popping up on the panel.","Accommodation","Communication","Equipment Related","10.28","Low","","","Telephone exchange noticed No alarm. ","2020-04-23T23:59:17","DEUR190078","Completed","2020-05-03T23:59:17","No","No","No","Internal","Target date revised due to lead time of spares."]
[null,null,null,6265,null,"88_20/11/2019 2:19:15 PM","2019-12-13T23:59:17","Defect","Ship Staff","Ship Staff Insp.","Washing Machine in ship Laundry to be repaired","Elect. Mach. & Equip.","MLC Related","Equipment Related","11.14","Medium","","","Vessel need Door and spares for same.RO DEUR190014 Raised","2020-02-23T23:59:17","DEUR190014","Completed","2020-02-11T23:59:17","No","No","No","Internal","Will be supplied at next convenient port."]
[null,null,null,2263,null,"88_17/10/2019 1:43:27 PM","2019-12-19T23:59:17","Defect","Ship Staff","Ship Staff Insp.","Port side forward Vapor return line manifold valve worm gear damaged / worn out completely.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.25","Very High","","","Renew worm gear / valve","2020-03-10T23:59:17","","Completed","2020-03-12T23:59:17","Yes","No","No","Internal","Raise RO for worm gear valve"]
[null,null,null,9544,null,"88_10/1/2020 4:59:43 AM","2019-12-26T23:59:17","Observation","Ship Staff","Ship Staff Insp.","Pressure gauges in CCR for ballast found showing erratic readings during loading operations.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.12","Medium","","","All pressure and compound gauges in pump room calibrated and adjusted with pressure calibrator. All gauges showing similar readings in pump room and CCR.","2020-02-10T23:59:17","","Completed","2020-01-04T23:59:17","No","No","No","Internal"]
[null,null,null,9545,null,"88_10/1/2020 5:03:05 AM","2019-12-26T23:59:17","Observation","Ship Staff","Ship Staff Insp.","Helicopter area on main deck noticed to be without anti skid paint.","Miscellaneous","General Appearance","Inappropriate Procedure","11.3","Medium","","","Vessel carried out chipping and painting of area followed by painting of entire area with anti skid.","2020-02-10T23:59:17","","Completed","2020-01-05T23:59:17","No","No","No","Internal"]
[null,null,null,9548,null,"88_10/01/2020 17:23:43","2020-01-01T23:59:17","Other","Ship Staff","Ship Staff Insp.","All CFL  lights in accomodation to be replaced with LED. Capacitors to be removed from the circuit","Accommodation ","General Appearance","Industry Issue","11.1","High","","","All CFL  lights replaced with LED, and Capacitors removed from the circuit.","2020-08-26T23:59:17","","Completed","2020-08-21T23:59:17","No","No","No","Internal","How much  % remaining."]
[null,null,null,9870,null,"88_20/01/2020 10:27:21","2020-01-08T23:59:17","Observation","Ship Staff","Ship Staff Insp.","ME Turning gear shaft seal leaking during operation","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.35","Very High","","","Defect has been added to REFMAN,To be attended in Dry dock. Job closed as instruction from office","2021-01-26T23:59:17","","Completed","2020-12-15T23:59:17","No","No","No","Internal","I believe vessel has already received the spares."]
[null,null,null,10388,null,"88_02-02-2020 12:35:42","2020-01-26T23:59:17","Defect","Ship Staff","Ship Staff Insp.","Boiler #1 atomising steam valve operation erratic","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.34","High","","","Boiler #1 atomising steam controller erratic operation to be investigated","2020-02-23T23:59:17","","Completed","2020-02-24T23:59:17","No","No","No","Internal"]
[null,null,null,10389,null,"88_02-02-2020 12:33:38","2020-01-26T23:59:17","Defect","Ship Staff","Ship Staff Insp.","IG uptake #2 valve hard to operate.","Inert Gas","Eng. / Strg. Comp.","Equipment Related","10.35","Very High","","","IG uptake #2 valve to be checked for free operation/ Valve removed from place eased up and put back. Tried out found working satisfactorily.","2020-03-10T23:59:17","","Completed","2020-02-28T23:59:17","No","No","No","Internal","Please attend this job ASAP. IT may create problem during discharging operaion."]
[null,null,null,10390,null,"88_02-02-2020 12:37:46","2020-01-26T23:59:17","Defect","Ship Staff","Ship Staff Insp.","Main SW pump #3 leak from mechanical seal","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.33","High","","","Main SW pump #3 leak from mechanical seal due to muddy waters. Mechanical seal to be renewed","2020-02-23T23:59:17","","Completed","2020-02-01T23:59:17","No","No","No","Internal"]
[null,null,null,10391,null,"88_3/2/2020 12:21:34 AM","2020-01-28T23:59:17","Defect,Observation","Ship Staff","Ship Staff Insp.","IG vent valve (pneumatic) found not closing completely while IGS in operation.","Inert Gas","Cargo / Ballast Systems","Equipment Related","8.19","High","","","Ig vent valve dismantled and found pneumatic actuator not closing completely. Overhauling of actuator & adjustment carried out. Vent valve fixed back with renewed flame screen.","2020-02-23T23:59:17","","Completed","2020-02-04T23:59:17","No","No","No","Internal"]
[null,null,null,10392,null,"88_3/2/2020 12:23:28 AM","2020-01-28T23:59:17","Observation","Ship Staff","Ship Staff Insp.","PV breaker sight glass found to be cracked during cargo operations.","Inert Gas","Cargo / Ballast Systems","Equipment Related","8.36","Medium","","","PV breaker glass (Acrylic sheet) renewed.","2020-02-23T23:59:17","","Completed","2020-01-31T23:59:17","No","No","No","Internal"]
[null,null,null,10693,null,"88_29/2/2020 7:55:26 AM","2020-02-03T23:59:17","Defect,Observation","Ship Staff","Ship Staff Insp.","Supporting rings for the wire mesh on vaccumm side for PV valves found to be wasted and broken from several locations.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.21","High","","","Supporting rings are being dismantled and repair works being carried out in by hot work.","2020-03-15T23:59:17","","Completed","2020-03-15T23:59:17","No","No","No","Internal"]
[null,null,null,10694,null,"88_29/2/2020 7:51:55 AM","2020-02-05T23:59:17","Defect,Observation","Ship Staff","Ship Staff Insp.","Ballast tank vent head fins observed to be wasted and broken from locations","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.53","Low","","","All ballast tank vent heads fins renewed and fixed back at location.","2020-05-25T23:59:17","","Completed","2020-05-24T23:59:17","No","No","No","Internal","How many vent heads are remaining for repair."]
[null,null,null,10533,null,"88_16/02/2020 02:26:16","2020-02-06T23:59:17","Observation","Ship Staff","Ship Staff Insp.","Main Air compressor #1 FW inlet valve not holding, job to be carried out at Anchorage. Vessel has spare valve on board.","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related","10.34","High","","","Main Air compressor #1 FW inlet valve not holding, job to be carried out at safe anchorage. Vessel has spare valve on board.","2020-04-08T23:59:17","","Completed","2020-03-24T23:59:17","No","No","No","Internal","Does vessel have the spare valve, or raise RO."]
[null,null,null,10535,null,"88_16/02/2020 02:33:50","2020-02-07T23:59:17","Observation","Ship Staff","Ship Staff Insp.","Cascade tank level gauge cracked","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Level gauge to be repaired","2020-02-24T23:59:17","","Completed","2020-02-17T23:59:17","No","No","No","Internal"]
[null,null,null,10695,null,"88_29/2/2020 2:06:17 PM","2020-02-23T23:59:17","Observation","Owner / Marine / Tech. Suptd.","Cargo Audit","Pre arrival check list section B time not entered.","Documentation","Cargo / Ballast Systems","Human Error,Inappropriate Procedure","8.1","Very High","","","Time entered for relevant section","2020-02-23T23:59:17","","Completed","2020-02-23T23:59:17","No","No","No","Internal"]
[null,null,null,10696,null,"88_29/2/2020 2:55:25 PM","2020-02-23T23:59:17","Observation","Owner / Marine / Tech. Suptd.","Cargo Audit","Discharging Zhoushan - LIne set up was not cross checked by two officers. Line set up was cross checked by 3rd officer only.","Documentation","Cargo / Ballast Systems","Human Error,Inappropriate Procedure","8.6","Medium","","","Correct entry made and same rectified in the CCR log book","2020-02-23T23:59:17","","Completed","2020-02-23T23:59:17","No","No","No","Internal"]
[null,null,null,10697,null,"88_01-03-2020 22:25:14","2020-02-23T23:59:17","Observation","Owner / Marine / Tech. Suptd.","Bunkering Audit","Benzene reading to be recorded < than minimum recording on the tube if it shows zero reading.","Documentation","Eng. / Strg. Comp.","Inappropriate Procedure","10.8","Medium","","","Corrected in the last bunker checklist and all officers trained regarding the same.","2020-02-24T23:59:17","","Completed","2020-02-24T23:59:17","No","No","No","Internal"]
[null,null,null,10769,null,"88_15/3/2020 4:58:36 AM","2020-03-05T23:59:17","Defect,Observation","Ship Staff","Ship Staff Insp.","Controller for MW#3 found to be leaking.","Deck - Mooring Machinery","Mooring","Equipment Related","9.14","Medium","","","Received the controller under RO DEUR200089. Vessel staff has fixed the controller and tried out. No leaks noticed. to be monitored during mooring operations while wire is on load.","2020-05-26T23:59:17","DEUR200089","Completed","2020-05-07T23:59:17","No","No","No","Internal"]
[null,null,null,10770,null,"88_15/3/2020 10:02:27 PM","2020-03-05T23:59:17","Observation","Ship Staff","Ship Staff Insp.","Gratings on port side provision crane winch platform found broken","Deck - Machinery","Cargo / Ballast Systems","Equipment Related","8.5","Very High","","","To replace the grating after seeking concurrence from office for working aloft.","2020-03-15T23:59:17","","Completed","2020-03-17T23:59:17","No","No","No","Internal"]
[null,null,null,10771,null,"88_15/3/2020 5:02:39 AM","2020-03-07T23:59:17","Defect,Observation","Ship Staff","Ship Staff Insp.","Oil leaks noticed from port side midship crane oil level gauge glass","Deck - Machinery","Cargo / Ballast Systems","Equipment Related","8.5","Very High","","","Vessel will drain the oil from port side midship crane to carry out repairs on the gauge glass. Oil level to be renewed back to normal on completion of repairs.","2020-03-15T23:59:17","","Completed","2020-03-16T23:59:17","No","No","No","Internal"]
[null,null,null,11056,null,"88_1/4/2020 7:21:26 AM","2020-03-12T23:59:17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","All gratings for crane platforms to be renewed with new gratings.","Deck - Machinery","General Appearance","Equipment Related","8.5","Very High","","","Renewed all gratings for port side provision craneand stbd side provision crane carried out.","2020-06-10T23:59:17","DEUR200079","Completed","2020-05-27T23:59:17","No","No","No","Internal"]
[null,null,null,11051,null,"88_31/03/2020 07:09:05","2020-03-18T23:59:17","Defect,Observation","Ship Staff","Ship Staff Insp.","ME Unit No.4 VIT stuck at 8.9 as compare to other units around 5.0 causing unit no.4 high peak pressure.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","We tried to free up the VIT but VIT doesn't move and is stuck at 8.9 and is not coming below 8.9 as compare to other units around 5.0, causing Unit no. 4 High peak pressure.                  ACTION TAKEN: Fuel pump overhauled and balancing carried out between units, performance taken found all units well balanced and VIT racks same for all units.","2020-05-24T23:59:17","","Completed","2020-09-29T23:59:17","No","No","No","Internal"]
[null,null,null,11052,null,"88_1/4/2020 7:25:22 AM","2020-03-22T23:59:17","Defect,Observation","Ship Staff","Ship Staff Insp.","VECS manifold valves found to be leaking and not holding","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.3","Very High","","","Vessel completed job in dry dock.","2021-04-10T23:59:17","","Completed","2021-03-23T23:59:17","No","No","No","Internal","Supplied ring was found to be of wrong size.  Correct size  seat ring will be supplied  by end of Jan. Target date revised accordingly."]
[null,null,null,16662,null,"88_4/1/2021 11:36:00 PM","2020-03-24T23:59:17","Observation","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","Air bubble was found in the standard magnetic compass bowl located in the compass bridge deck.","Navigation - Others","Navigation","Equipment Related","4.9","Medium","","","It was rectified before the inspector's disembarkation.","2020-03-24T23:59:17","","Completed","2020-03-24T23:59:17","No","No","No","External"]
[null,null,null,11053,null,"88_1/4/2020 7:30:13 AM","2020-03-25T23:59:17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Platform nut & bolts on crane to be renewed with SUS 316 grade nut & bolts.","Deck - Machinery","Structural Condn. / WT integrity ","Equipment Related","8.5","Very High","","","Platform nuts & bolts inspected while carrying out wire renewal for crane and found to be of stainless steel material. Change of nut & bolts not required.","2020-08-26T23:59:17","","Completed","2020-08-12T23:59:17","No","No","No","Internal","Job to be attended in loaded passage.  Target date revised."]
[null,null,null,11054,null,"88_31/03/2020 06:34:58","2020-03-26T23:59:17","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Spares inventory of machineries and other related is not updated in PAL PMS same to be updated before 30 June 2020","Documentation","ISM Related","Equipment Related","10.12","Very High","","","Updating of spares in PAL PMS is completed.","2020-06-25T23:59:17","","Completed","2020-06-25T23:59:17","No","No","No","Internal"]
[null,null,null,11055,null,"88_1/4/2020 7:36:16 AM","2020-03-27T23:59:17","Defect","Ship Staff","Ship Staff Insp.","Cargo pump no. 3 had been reported to leak slightly from upper mechanical seal since take over. Same was checked during last discharge with a light crude oil and confirmed.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.8","Medium","","","Upper and lower mechanical seals renewed. COP fixed back and tried out at 850 RPM with a discharge pressure of 10.0 bars. No leaks noticed from the upper mech. seal. To be observed further during actual discharging.","2020-05-10T23:59:17","","Completed","2020-05-06T23:59:17","No","No","No","Internal"]
[null,null,null,10768,null,"88_15/3/2020 4:54:59 AM","2020-04-04T23:59:17","Observation","Ship Staff","Ship Staff Insp.","Sounding pipes for 5S WBT found to be choked.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.13","Medium","","","5S WBT sounding pipe is a seamless pipe. Vessel staff tried to clear the choke from pump room but in vain. Will have to be attended in dry dock.","2020-07-10T23:59:17","","Completed","2020-07-10T23:59:17","Yes","No","No","Internal"]
[null,null,null,11457,null,"88_16/4/2020 8:51:02 AM","2020-04-05T23:59:17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Stbd provision crane starter box cover is damaged. needs to be fixed.","Deck - Machinery","General Appearance","Equipment Related","8.1","Very High","","","To fabricate a new cover for the existing box at place","2020-04-15T23:59:17","","Completed","2020-04-10T23:59:17","No","No","No","Internal"]
[null,null,null,11458,null,"88_16/4/2020 8:54:23 AM","2020-04-05T23:59:17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Fore peak store stbd side bulkheads needs to be cleaned and painted as same found in dirty condition.","Accommodation","General Appearance","External Factors","11.3","Medium","","","Washing and cleaning of forward store areas carried out.","2020-04-25T23:59:17","","Completed","2020-05-03T23:59:17","No","No","No","Internal"]
[null,null,null,11459,null,"88_16/4/2020 8:59:16 AM","2020-04-05T23:59:17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","To segregate discarded ropes and tag them for easy identification in the forward store","Miscellaneous","General Appearance","External Factors","11.3","Medium","","","Discarded ropes in forward store arranged and kept properly. Discarded rpes have been tagged also.","2020-04-25T23:59:17","","Completed","2020-05-03T23:59:17","No","No","No","Internal"]
[null,null,null,11460,null,"88_16/4/2020 9:04:37 AM","2020-04-05T23:59:17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Understand that PV breaker sight glass needs to be renewed very frequently as sam e getting cracked. Order proper spares from manual.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.28","Medium","","","Vessel received the spare on 17 Sept 2020 at singapore and same was renewed at location.","2020-09-25T23:59:17","","Completed","2020-09-14T23:59:17","No","No","No","Internal",""]
[null,null,null,13020,null,"88_5/7/2020 11:10:18 PM","2020-04-05T23:59:17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","In pump room stbd side there is drop leak from one of the bunker line pipe.  Oil drop can be seen on the bulkhead. Flanges to tight or gasket to renew if required. ","Deck - Pipe / Fittings","MARPOL Related","Equipment Related","6.8","High","","","The flange for engine room sludge transfer to slop stbd was tightened and leak arrested. Leftover fuel from the line also drained to avoid leak due to expansion.","2020-04-12T23:59:17","","Completed","2020-04-12T23:59:17","No","No","No","Internal"]
[null,null,null,13021,null,"88_6/7/2020 7:23:24 PM","2020-04-05T23:59:17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Leak sighted from the connections of pressure gauges of steering gear pumps. To rectify.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Pressure gauge connections tightened; leaks rectified.","2020-05-05T23:59:17","","Completed","2020-04-06T23:59:17","No","No","No","Internal"]
[null,null,null,13022,null,"88_6/7/2020 7:26:06 PM","2020-04-05T23:59:17","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Aft most Top bracing to fit back in place.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Top bracing fitted back.","2020-05-05T23:59:17","","Completed","2020-04-16T23:59:17","No","No","No","Internal"]
[null,null,null,13023,null,"88_6/7/2020 7:30:17 PM","2020-04-05T23:59:17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Vent head at China Passage( FO Overflow Tank, ME LO settling tank, OBT and Hotwell) are in bad shape. Cleaning and painting required.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","11.3","Medium","","","Vent heads cleaned and painted.","2020-04-20T23:59:17","","Completed","2020-04-17T23:59:17","No","No","No","Internal"]
[null,null,null,13024,null,"88_6/7/2020 7:34:06 PM","2020-04-05T23:59:17","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Hand phone set in workshop is in bad condition. Insulation tape has been used to repair it and even sound is not audible. To replce.","Elect. Mach. & Equip.","Communication","Equipment Related","10.28","Low","","","Phone rectified. Presently working fine.","2020-05-05T23:59:17","","Completed","2020-04-10T23:59:17","No","No","No","Internal"]
[null,null,null,13025,null,"88_6/7/2020 7:45:28 PM","2020-04-05T23:59:17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","220V insulation found to be only 0.7 Mohm in port. To rectify.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.24","Low","","","220V insulation rectified. ","2020-04-25T23:59:17","","Completed","2020-04-20T23:59:17","No","No","No","Internal"]
[null,null,null,13026,null,"88_6/7/2020 7:37:39 PM","2020-04-05T23:59:17","Defect","Owner / Marine / Tech. Suptd.","Ship Staff Insp.","While inspecting hull, no water flow was sighted for rudder neck bearing. To check the pipe for blockage.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.28","Low","","","Dry Dock Job.Raised in Refman","2020-04-20T23:59:17","","Completed","2020-06-29T23:59:17","No","No","No","Internal"]
[null,null,null,13027,null,"88_06/07/2020 15:26:51","2020-04-05T23:59:17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Engine room vacuum toilet parts are not secured in place, flush switch is missing. To rectify.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Flush switch fitted in place, rectified.","2020-04-15T23:59:17","","Completed","2020-04-13T23:59:17","No","No","No","Internal"]
[null,null,null,13028,null,"88_06/07/2020 15:59:09","2020-04-05T23:59:17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Stbd provision crane slewing motion limit switch is broken and lying on floor. To rectify and test all limits of crane.","Deck - Machinery","Cargo / Ballast Systems","Equipment Related","8.23","Medium","","","Stbd provision crane slewing motion limit switch put in place rectified, tested all limits of crane found working satisfactory.","2020-04-15T23:59:17","","Completed","2020-04-09T23:59:17","No","No","No","Internal"]
[null,null,null,10534,null,"88_16/02/2020 02:30:33","2020-04-07T23:59:17","Observation","Ship Staff","Ship Staff Insp.","FW expansion tank level gauge slight leak","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.33","High","","","Gauge glass renewed. Gland packings for valves renewed with teflon cord.","2020-09-25T23:59:17","","Completed","2020-10-07T23:59:17","No","No","No","Internal","Long anchorage required for the job"]
[null,null,null,11461,null,"88_16/4/2020 9:07:44 AM","2020-04-09T23:59:17","Observation","Ship Staff","Ship Staff Insp.","Hydraulic return line on MW#5 found to be leaking.","Deck - Mooring Machinery","Mooring","Equipment Related","9.14","Medium","","","Pipe section removed from location and repairs carried out on pipe section  in work shop. Pipe section fixed back at location and tried out. No leaks observed. Clamps for the hydraulic line renewed.","2020-04-15T23:59:17","","Completed","2020-04-18T23:59:17","No","No","No","Internal","Has it not yet  beencomplete?"]
[null,null,null,11580,null,"88_29/4/2020 6:16:41 AM","2020-04-20T23:59:17","Observation","Ship Staff","Ship Staff Insp.","Port side midship draft gauge not working since take over. Showing an erratic reading.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.15","High","","","Job added in REFMAN","2020-09-25T23:59:17","DEUR200128","Completed","2020-08-31T23:59:17","No","No","No","Internal","Job to be attended during docking. Shift it in refman"]
[null,null,null,11579,null,"88_30/4/2020 3:22:26 PM","2020-04-21T23:59:17","Defect","Ship Staff","Ship Staff Insp.","Inlet SW pipe for forward mooring LO cooler found holed while in operation.","Deck - Mooring Machinery","Mooring","Equipment Related","11.5","Medium","","","Pipe section removed and repairs carried out on the pipe in the workshop. Pipe section fixed back at Location and tried out. No leaks.","2020-05-10T23:59:17","","Completed","2020-05-02T23:59:17","No","No","No","Internal"]
[null,null,null,11822,null,"88_14/5/2020 5:39:15 AM","2020-04-30T23:59:17","Defect,Observation","Ship Staff","Ship Staff Insp.","06 No.s COT PV valves noticed to be leaking from pressure and vaccumm side when checked by personal gas meters.","Inert Gas","Cargo / Ballast Systems","Equipment Related","8.41","Medium","","","Vessel staff carried out lapping & overhauling of all 6 PV valves. Noticed magnets in worn out condition.","2020-05-25T23:59:17","","Completed","2020-05-22T23:59:17","No","No","No","Internal"]
[null,null,null,11823,null,"88_14/5/2020 5:43:40 AM","2020-05-04T23:59:17","Observation","Ship Staff","Ship Staff Insp.","Port side windlass found again slow after adjustment of throttle valve, It was ok as per the requirement while anchor at PAL, but as reported slow again during next anchor operation.No such issues while heaving up the anchor","Deck - Mooring Machinery","Mooring","Equipment Related","9.2","Very High","","","Speed checked again and found satisfactory.","2020-07-15T23:59:17","","Completed","2020-07-08T23:59:17","No","No","No","Internal","Please do the excercise again as advised  by maker"]
[null,null,null,11825,null,"88_14/5/2020 5:30:50 AM","2020-05-05T23:59:17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Butterworth covers found leaking aroung cap nuts.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.58","High","","","The cap nuts were found to be worn out during opening of manholes while carrying out tank cleaning operations. The cap nuts were received on 09 May 2020. All loose thread cap nuts have been replaced with new cap nuts and leaks arrested.","2020-05-10T23:59:17","","Completed","2020-05-08T23:59:17","No","No","No","Internal"]
[null,null,null,11824,null,"88_14/5/2020 5:22:26 AM","2020-05-07T23:59:17","Defect","Ship Staff","Ship Staff Insp.","IG NRV opened up foir inspection and found NRV flap seized at about 10% open condition. Valve drain flange found holed and shaft stopper ring found damaged.","Inert Gas","Cargo / Ballast Systems","Equipment Related","8.23","Medium","","","Vessal staff to carry out complete overhauling of the NRV. Holed flange to repaired. Stopper rings to be renewed and flap to be made free.","2020-05-11T23:59:17","","Completed","2020-05-11T23:59:17","No","No","No","Internal"]
[null,null,null,11966,null,"88_27/5/2020 3:24:14 AM","2020-05-11T23:59:17","Breakdown","Ship Staff","Ship Staff Insp.","COW machine for 5S (fwd) found broken from stand pipe and fallen at tank bottom","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.34","High","","","Vessel renewed the COW machine unit which was supplied on 17 Sept 2020   @ Singapore.","2020-09-25T23:59:17","DEUR200103","Completed","2020-09-14T23:59:17","No","No","No","Internal","Awaiting supply of spares. Target date revised accordingly."]
[null,null,null,16648,null,"88_4/1/2021 7:07:16 PM","2020-06-05T23:59:17","Observation","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","GMDSS Batteries located on the bridge was observed that the shelf life of the batteries was less than (2) years(03 will expire in Apr 2021whereas another 3 will expire in Oct 2021) not in accordance with IMO MSC.149 (77)","Navigation - GMDSS & Communication","Navigation","Equipment Related","4.27","High","","","As per IMO MSC.149(77), Primary batteries should have a shelf life of at least 2 years, and if identified to be user replaceable should be of a colour or marking as defined in 2.3.13.","2020-07-05T23:59:17","","Completed","2020-06-09T23:59:17","No","No","No","External"]
[null,null,null,12971,null,"88_30/6/2020 1:24:15 AM","2020-06-15T23:59:17","Breakdown,Defect","Ship Staff","Ship Staff Insp.","During last STS operations vessel found oil leaking from tapping of eductor gauge from the diffuser of the cargo eductor. On inspection it was noticed that the same had been welded before.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.8","Medium","","","vessel staff has disconnected the diffuser of the eductor and landed same in the engine workshop for renewal of thread and coupling. On completionof repairs same to be fixed back at location.","2020-07-05T23:59:17","","Completed","2020-07-02T23:59:17","No","No","No","Internal"]
[null,null,null,12972,null,"88_30/6/2020 1:28:27 AM","2020-06-20T23:59:17","Defect","Ship Staff","Suptd. Insp.","During deck rounds vessel staff noticed leak from one section of deck air line i.w.o of the securing clamp.","Deck - Machinery","Mooring","Equipment Related","11.5","Medium","","","Vessel staff to remove the air pipe section and give it to the workshop for repairs on the pipe section.","2020-07-10T23:59:17","","Completed","2020-07-03T23:59:17","No","No","No","Internal"]
[null,null,null,12973,null,"88_30-06-2020 06:49:38","2020-06-21T23:59:17","Defect","Ship Staff","Ship Staff Insp.","ME Unit no. 5 Fuel pump VIT rack found stuck at 9.8 due to which No. 5 unit shows highpeak pressure during ME performance.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Fuel pump replaced with overhauled onbaord, Performance taken found working satisfactory. ","2020-09-25T23:59:17","","Completed","2020-09-12T23:59:17","No","No","No","Internal","Job to be attended at Singapore. Target date revised."]
[null,null,null,12974,null,"88_30-06-2020 01:36:44","2020-06-21T23:59:17","Observation","Ship Staff","Ship Staff Insp.","Noted ME Unit no. 2 Fuel pipe leaking from top of fuel pump joint connection.","E/R - Pipes/ valves & fittings","Safety / LSA / FFA","Equipment Related","10.31","Very High","","","Taken out the pipe lapping of surface carrie out fitted back found no leak.","2020-06-21T23:59:17","","Completed","2020-06-21T23:59:17","No","No","No","Internal"]
[null,null,null,13019,null,"88_6/7/2020 1:29:31 AM","2020-06-26T23:59:17","Defect,Observation","Ship Staff","Ship Staff Insp.","Port side provision crane hyraulic cylinder found to be leakng from the upper seals","Deck - Machinery","MARPOL Related","Equipment Related","8.5","Very High","","","Defect has been added to REMAN. TO be attended to during dry dock. Job closed as per instruction from office","2021-01-26T23:59:17","","Completed","2020-12-15T23:59:17","Yes","No","No","Internal"]
[null,null,null,13171,null,"88_10/07/2020 09:31:13","2020-07-01T23:59:17","Breakdown","Ship Staff","Ship Staff Insp.","During mothly crank case inspection noticed, Top up air compressor LP Piston gudgeon pin bush grab screw found slack which damaged the LP Gudgeon pin, LP top needle bearings and LP Con rod. ","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","All the defective parts like LP piston Gudgeon pin, LP top needle bearings and LP Con rod renewed. Air compressor tried out, working satisfactory.","2020-07-07T23:59:17","","Completed","2020-07-07T23:59:17","No","No","No","Internal"]
[null,null,null,13246,null,"88_31/07/2020 10:50:02","2020-07-20T23:59:17","Defect,Observation","Ship Staff","Ship Staff Insp.","COP No.2 Governor oil leakage from the power cylinder due to seal damaged.","Cargo Mach.","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Spare Governor received while passing Singapore fitted in place and to tried out found working properly.","2020-08-26T23:59:17","DEUR200158","Completed","2020-08-13T23:59:17","No","No","No","Internal","Governor already supplied."]
[null,null,null,13517,null,"88_06/08/2020 11:29:31","2020-08-01T23:59:17","Defect","Ship Staff","Ship Staff Insp.","M/E Fuel testing equipment noticed not building up pressuredue to Hydraulic piston seal damaged.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.31","Very High","","","DEUR200156 spartes received at Singapore equipment parts changed found working satisfactory.","2020-09-17T23:59:17","","Completed","2020-09-16T23:59:17","No","No","No","Internal","Will be supplied at next call Singapore."]
[null,null,null,13773,null,"88_31/08/2020 15:24:02","2020-08-24T23:59:17","Defect","Ship Staff","Ship Staff Insp.","During routine inspection found the boiler expansion bellow fitted in the  smoke uptake damaged.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.31","Very High","","","Spare bellow received at Singapore on 17 Sept 2020 job completed in DD.","2021-03-20T23:59:17","","Completed","2021-03-13T23:59:17","Yes","No","No","Internal"]
[null,null,null,13949,null,"88_15/9/2020 10:23:46 AM","2020-09-01T23:59:17","Defect","Ship Staff","Ship Staff Insp.","COW machine for 1P (aft) found not operating during COW operations at discharge port.","Cargo Mach.,Deck - Machinery","Cargo / Ballast Systems","Equipment Related","8.34","High","","","Vessel inspected the drive unit and found all satisfactory.Drive unit overhauled and found satisfactory. Operation to be checked at the next discharge port ","2020-11-25T23:59:17","","Completed","2020-11-13T23:59:17","No","No","No","Internal"]
[null,null,null,13950,null,"88_11/09/2020 11:13:15","2020-09-02T23:59:17","Defect","Ship Staff","Ship Staff Insp.","Fire & GS Pump found mechanical seal leaking.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Fire & GS Pump removed from place and bought to workshop Mech seal renewed, Motor connections made, Pump to be tried out.","2020-09-09T23:59:17","","Completed","2020-09-06T23:59:17","No","No","No","Internal"]
[null,null,null,14414,null,"88_12/10/2020 1:04:44 AM","2020-09-12T23:59:17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Pipes on main deck support angle bars rusted","Deck - Pipe / Fittings","Eng. / Strg. Comp.","Equipment Related","11.4","Very High","","","Pipes on main deck support angle bars rusted derusted and painted","2020-12-12T23:59:17","","Completed","2020-11-12T23:59:17","No","No","No","Internal"]
[null,null,null,14415,null,"88_12/10/2020 12:57:15 AM","2020-09-12T23:59:17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Pipes on main deck rusted iwo U clamps, to de-rust and paint","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.5","Medium","","","Pipes on main deck de- rusted iwo U clamps and painted.","2020-12-12T23:59:17","","Completed","2020-11-28T23:59:17","No","No","No","Internal"]
[null,null,null,14416,null,"88_12/10/2020 1:01:09 AM","2020-09-12T23:59:17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Pipes on main deck rusted, to de-rust and paint","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.4","Very High","","","Pipes on main deck derusted and painted","2020-12-25T23:59:17","","Completed","2020-11-15T23:59:17","No","No","No","Internal"]
[null,null,null,14417,null,"88_12/10/2020 1:03:33 AM","2020-09-12T23:59:17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Ballast tanks dome cover packing channel outer lip rusted","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.7","High","","","Ballast tanks dome cover packing channel outer lip derusted and painted","2020-12-12T23:59:17","","Completed","2020-11-29T23:59:17","No","No","No","Internal"]
[null,null,null,14418,null,"88_12/10/2020 1:06:16 AM","2020-09-12T23:59:17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Mooring winches hydraulic pipe thinned iwo U clamps, to renew","Deck - Pipe / Fittings","Mooring","Equipment Related","11.4","Very High","","","Shifted to Refman","2020-12-12T23:59:17","","Completed","2020-09-15T23:59:17","No","No","No","Internal"]
[null,null,null,14419,null,"88_12/10/2020 10:38:51 AM","2020-09-12T23:59:17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Gangway (S) davit stained – to de-rust and paint","Deck - Machinery","General Appearance","Equipment Related","11.3","Medium","","","Gangway (S) davit de-rusted and painted ","2020-11-25T23:59:17","","Completed","2020-11-16T23:59:17","No","No","No","Internal"]
[null,null,null,14420,null,"88_12/10/2020 10:51:51 AM","2020-09-12T23:59:17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","MW hydraulic pipe support angle bar wasted","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.4","Very High","","","MW hydraulic pipe support angle bar renewed.","2021-02-10T23:59:17","","Completed","2020-11-07T23:59:17","No","No","No","Internal"]
[null,null,null,14422,null,"88_12/10/2020 10:54:26 AM","2020-09-12T23:59:17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Slop tanks steam heating coils deck penetration pipe to de-rust","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.4","Very High","","","Slop tanks steam heating coils deck penetration pipe de rusted and painted ","2020-11-25T23:59:17","","Completed","2020-11-14T23:59:17","No","No","No","Internal"]
[null,null,null,14423,null,"88_12/10/2020 10:56:47 AM","2020-09-12T23:59:17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Slop tank (P) steam heating pipe support angle bar wasted","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.4","Very High","","","new angle bar bolted.","2021-02-10T23:59:17","","Completed","2020-10-16T23:59:17","No","No","No","Internal"]
[null,null,null,14424,null,"88_12/10/2020 10:58:05 AM","2020-09-12T23:59:17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","‘A’ deck port side drain pipe wasted, to renew ","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.4","Very High","","","‘A’ deck port side drain pipe renewed","2021-02-10T23:59:17","","Completed","2020-11-03T23:59:17","No","No","No","Internal"]
[null,null,null,14426,null,"88_12/10/2020 10:47:39 AM","2020-09-12T23:59:17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Main deck plating spot rust to de-rust and paint","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.3","Medium","","","Main deck plating spot rust  de-rusted and painted","2020-12-25T23:59:17","","Completed","2020-11-30T23:59:17","No","No","No","Internal"]
[null,null,null,14427,null,"88_12/10/2020 12:59:36 AM","2020-09-12T23:59:17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Electrical cable support channel connector piece missing","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.4","Very High","","","Electrical cable support channel connector piece renewed","2020-11-25T23:59:17","","Completed","2020-11-19T23:59:17","No","No","No","Internal"]
[null,null,null,14428,null,"88_12/10/2020 1:09:53 AM","2020-09-12T23:59:17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Windlass hydraulic pump motor panel curtain not secured properly to hooks","Deck - Mooring Machinery","General Appearance","Equipment Related","10.23","Medium","","","Curtain secured back properly on the bar","2020-09-19T23:59:17","","Completed","2020-10-02T23:59:17","No","No","No","Internal"]
[null,null,null,14429,null,"88_12/10/2020 10:41:43 AM","2020-09-12T23:59:17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Windlass hydraulic pump motor panel curtain not secured properly to hooks","Deck - Mooring Machinery","General Appearance","Equipment Related","10.23","Medium","","","New hooks put in place and secured properly to the curtain bar","2020-10-05T23:59:17","","Completed","2020-10-02T23:59:17","No","No","No","Internal"]
[null,null,null,14430,null,"88_12/10/2020 10:50:30 AM","2020-09-12T23:59:17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","COT 4 (S) & 5 (S) - traces of vapour escape from dome cover. To investigate and renew packing. ","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.3","Medium","","","Tightened the Tank dome covers for No 4Sand 5S COT. No leaks observed","2020-10-05T23:59:17","","Completed","2020-10-02T23:59:17","No","No","No","Internal"]
[null,null,null,14431,null,"88_12/10/2020 10:59:27 AM","2020-09-12T23:59:17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Crew recreation room curtains not secured to hooks\n\n\n\n","Accommodation","General Appearance","Equipment Related","11.13","Low","","","Curtains secured to the hooks properly","2020-10-05T23:59:17","","Completed","2020-10-02T23:59:17","No","No","No","Internal"]
[null,null,null,14432,null,"88_12/10/2020 11:01:16 AM","2020-09-12T23:59:17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","CO2 room air pipe cap missing","LSA / FFA","General Appearance","Equipment Related","11.6","Medium","","","Air pipe cap put back in place","2020-09-20T23:59:17","","Completed","2020-09-20T23:59:17","No","No","No","Internal"]
[null,null,null,14433,null,"88_12/10/2020 17:13:56","2020-09-12T23:59:17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Steering gear hydraulic pumps valve block minor oil leakage","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Leak rectified","2020-09-27T23:59:17","","Completed","2020-09-23T23:59:17","No","No","No","Internal"]
[null,null,null,14434,null,"88_13/10/2020 12:13:31 AM","2020-09-12T23:59:17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Aux Boiler (P) FO pipe lagging torn – to renewAux boiler (S) FO valve lagging torn     ","E/R - Pipes/ valves & fittings","General Appearance","Equipment Related","10.32","Very High","","","Lagging renewed","2020-09-19T23:59:17","","Completed","2020-09-19T23:59:17","No","No","No","Internal"]
[null,null,null,14435,null,"88_13/10/2020 12:19:43 AM","2020-09-12T23:59:17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Auxiliary boiler burner space to cleanSoot deposit on IG fans save all tray     ","E/R - Boiler","General Appearance","Equipment Related","10.32","Very High","","","Aux BLR burner space cleaned","2020-09-19T23:59:17","","Completed","2020-09-22T23:59:17","No","No","No","Internal"]
[null,null,null,14436,null,"88_13/10/2020 12:24:07 AM","2020-09-12T23:59:17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Aux boiler (S) FO valve lagging torn","E/R - Boiler","General Appearance","Equipment Related","10.32","Very High","","","Lagging renewed","2020-09-19T23:59:17","","Completed","2020-09-20T23:59:17","No","No","No","Internal"]
[null,null,null,14437,null,"88_13/10/2020 12:35:40 AM","2020-09-12T23:59:17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Soot deposit on IG fans save all tray to clean","Inert Gas","General Appearance","Equipment Related","10.32","Very High","","","Soot deposits cleaned","2020-09-19T23:59:17","","Completed","2020-09-20T23:59:17","No","No","No","Internal"]
[null,null,null,14438,null,"88_13/10/2020 12:40:26 AM","2020-09-12T23:59:17","Observation","Owner / Marine / Tech. Suptd.","Ship Staff Insp.","440V circuit earth meter (in emergency generator room) needle incorrectly adjusted","Critical Equip.","Emgcy. Systems","Equipment Related","10.38","Medium","","","Needle adjusted","2020-09-19T23:59:17","","Completed","2020-09-16T23:59:17","No","No","No","Internal"]
[null,null,null,14439,null,"88_13/10/2020 12:44:34 AM","2020-09-12T23:59:17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Aircon room weathertight door (at cross deck) wasted packing to renew","Miscellaneous","General Appearance","External Factors","11.6","Medium","","","packing renewed","2020-09-22T23:59:17","","Completed","2020-09-22T23:59:17","No","No","No","Internal"]
[null,null,null,14440,null,"88_12/10/2020 11:06:30 AM","2020-09-12T23:59:17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Aft peak tank air vent wire mesh missing","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.7","High","","","Wire mesh renewed and fitted","2020-09-22T23:59:17","","Completed","2020-10-02T23:59:17","No","No","No","Internal"]
[null,null,null,14441,null,"88_12/10/2020 11:08:59 AM","2020-09-12T23:59:17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Pump room steam line lagging stained – investigate and rectify","Deck - Pipe / Fittings","General Appearance","Equipment Related","8.44","High","","","Steam line lagging painted with HTA silver paint. So signs of oil stains. monitoring closely","2020-09-12T23:59:17","","Completed","2020-10-02T23:59:17","No","No","No","Internal"]
[null,null,null,14442,null,"88_13/10/2020 12:48:16 AM","2020-09-12T23:59:17","Observation","Owner / Marine / Tech. Suptd.","Ship Staff Insp.","Alfa Laval filter flange minor leakage to rectify","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Leakage rectified","2020-09-22T23:59:17","","Completed","2020-09-21T23:59:17","No","No","No","Internal"]
[null,null,null,14443,null,"88_13/10/2020 12:51:20 AM","2020-09-12T23:59:17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","A/E FO heater#1 steam inlet flange leakage to rectify","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Leakage rectified","2020-09-27T23:59:17","","Completed","2020-09-22T23:59:17","No","No","No","Internal"]
[null,null,null,14444,null,"88_13/10/2020 12:53:46 AM","2020-09-12T23:59:17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","M/E FO supply pump#1 leaking seal to replace","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Seal replaced","2020-09-27T23:59:17","","Completed","2020-09-24T23:59:17","No","No","No","Internal"]
[null,null,null,14445,null,"88_13/10/2020 12:56:06 AM","2020-09-12T23:59:17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","M/E FO circulating pump #2 pressure gauge connection minor leakage to rectify","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Leakage rectified","2020-09-19T23:59:17","","Completed","2020-09-18T23:59:17","No","No","No","Internal"]
[null,null,null,14446,null,"88_13/10/2020 12:59:31 AM","2020-09-12T23:59:17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","A/E# 3 charge air pressure gauge defective – to renew","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Pressure gauge renewed","2020-10-19T23:59:17","","Completed","2020-09-17T23:59:17","No","No","No","Internal"]
[null,null,null,14447,null,"88_13/10/2020 1:02:31 AM","2020-09-12T23:59:17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Soot tank overboard valve outboard flange has tell-tale sign of leakage","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Leakage rectified by tightening.","2020-10-12T23:59:17","","Completed","2020-09-22T23:59:17","No","No","No","Internal"]
[null,null,null,14448,null,"88_13/10/2020 1:04:46 AM","2020-09-12T23:59:17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Stern tube LO tank to mark for normal oil level to be maintained in the tank","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Normal level marked","2020-09-19T23:59:17","","Completed","2020-09-19T23:59:17","No","No","No","Internal"]
[null,null,null,14449,null,"88_13/10/2020 1:10:45 AM","2020-09-12T23:59:17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ECR floor matt dirty & stained","Miscellaneous","General Appearance","External Factors","10.32","Very High","","","Stains embedded into the venyl matting. Unable to clean. Rubber matting put on the ECR floor","2020-09-22T23:59:17","","Completed","2020-10-07T23:59:17","No","No","No","Internal"]
[null,null,null,14450,null,"88_12/10/2020 1:07:35 AM","2020-09-12T23:59:17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Bosun store deck plate at stairs landing rusted, to de-rust and paint","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.3","Medium","","","Bosun store deck plate at stairs landing de- rusted and painted","2020-10-12T23:59:17","","Completed","2020-10-12T23:59:17","No","No","No","Internal"]
[null,null,null,14451,null,"88_12/10/2020 10:55:39 AM","2020-09-12T23:59:17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Pump room ventilation fan cover to de-rust and paint","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.3","Medium","","","Pump room ventilation fan cover de-rusted and painted","2020-10-05T23:59:17","","Completed","2020-10-24T23:59:17","No","No","No","Internal"]
[null,null,null,14452,null,"88_12/10/2020 1:02:25 AM","2020-09-12T23:59:17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Pipes on main deck U clamp teflon packing cracked, to renew","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.5","Medium","","","Cracked teflon packing of U clamps renewed. ","2020-12-12T23:59:17","","Completed","2020-10-25T23:59:17","No","No","No","Internal"]
[null,null,null,14453,null,"88_12/10/2020 11:10:19 AM","2020-09-12T23:59:17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Sunken deck to steering gear entrance door packing channel at lower part rusted","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.6","Medium","","","Sunken deck to steering gear entrance door packing channel at lower part derusted and painted.","2020-10-15T23:59:17","","Completed","2020-10-10T23:59:17","No","No","No","Internal"]
[null,null,null,14454,null,"88_12/10/2020 11:02:58 AM","2020-09-12T23:59:17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","MW 6, 7 & 8- rope drum end plates to de-rust and paint ","Deck - Mooring Machinery","General Appearance","Equipment Related","11.3","Medium","","","MW 6, 7 & 8- rope drum end plates de-rusted and painted","2020-11-05T23:59:17","","Completed","2020-10-19T23:59:17","No","No","No","Internal"]
[null,null,null,14455,null,"88_12/10/2020 11:04:43 AM","2020-09-12T23:59:17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Steering gear skylight (at sunken deck) cover wasted packing lip to renew","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.3","Medium","","","Steering gear skylight (at sunken deck) cover wasted packing lip renewed, derusting and painting carried out","2020-11-05T23:59:17","","Completed","2020-10-12T23:59:17","No","No","No","Internal"]
[null,null,null,14456,null,"88_12/10/2020 10:43:44 AM","2020-09-12T23:59:17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Windlass (S) gear inspection cover not secured properly","Deck - Mooring Machinery","General Appearance","Equipment Related","9.14","Medium","","","Windlass (S) gear inspection cover secured properly","2020-10-05T23:59:17","","Completed","2020-10-08T23:59:17","No","No","No","Internal"]
[null,null,null,14457,null,"88_12/10/2020 10:45:13 AM","2020-09-12T23:59:17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Electrical conduit box on main deck rusted\n\n\n\n","Deck - Pipe / Fittings","General Appearance","Equipment Related","10.37","Medium","","","Electrical conduit box on main deck derusted\n\nand painted ","2020-10-05T23:59:17","","Completed","2020-10-12T23:59:17","No","No","No","Internal"]
[null,null,null,14458,null,"88_12/10/2020 10:46:21 AM","2020-09-12T23:59:17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Mooring winches rope drum end plates & linkages rusted, to de-rust and paint\n\n\n\n","Deck - Mooring Machinery","General Appearance","Equipment Related","11.3","Medium","","","Mooring winches rope drum end plates & linkages  de-rusted and painted","2020-10-12T23:59:17","","Completed","2020-10-19T23:59:17","No","No","No","Internal"]
[null,null,null,14034,null,"88_19/9/2020 3:19:14 PM","2020-09-14T23:59:17","Breakdown,Defect","Ship Staff","Ship Staff Insp.","the pump room gas detection system, oxygen sensor started to give a fault and showing a reading of 33.5% vol when the maximim range of measuring is 0-25%.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.46","Very High","","","Checked the sensor and found no change in the reading by adjusting the zero or span knobs on the sensor. to raise a RO for spare sensor. New sensor received at MIna Saqr. Same replaced and found working satisfactory.","2020-10-25T23:59:17","DEUR200190","Completed","2020-09-25T23:59:17","No","No","No","Internal"]
[null,null,null,14946,null,"88_23-11-2020 05:16:47","2020-11-09T23:59:17","Observation","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","The 2 laundry driers inspected each utilized thin plastic wlre ribbed collcertina type flexible pipes liable to trap any lint pass over and present a fire risk","Miscellaneous","General Appearance","Equipment Related","11.14","Medium","","","Plastic wlre ribbed collcertina type flexible pipes replaced with metal pipes, fabricated using galvanised metal sheets and lagged. ","2020-11-25T23:59:17","","Completed","2020-11-17T23:59:17","No","No","No","External"]
[null,null,null,16647,null,"88_29/12/2020 9:53:03 PM","2020-11-12T23:59:17","Observation","Owner / Marine / Tech. Suptd.","Ship Staff Insp.","Engine room aft casing stained - to clean and paint","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","External Factors","11.3","Medium","","","Engine aft casing bulkeads derusted & painted.","2021-04-25T23:59:17","","Completed","2021-03-15T23:59:17","No","No","No","Internal","Target date revised."]
[null,null,null,14421,null,"88_12/10/2020 10:53:03 AM","2020-11-15T23:59:17","Observation","Owner / Marine / Tech. Suptd.","Ship Staff Insp.","Accommodation front wall rust spots to de-rust and paint","Accommodation","General Appearance","Equipment Related","11.8","Low","","","Accomodation from rust spots derusted & painted whilst vessel in Yuilian drydock.","2021-04-25T23:59:17","","Completed","2021-03-20T23:59:17","Yes","No","No","Internal"]
[null,null,null,14425,null,"88_13/10/2020 1:07:55 AM","2020-11-21T23:59:17","Observation","Owner / Marine / Tech. Suptd.","Ship Staff Insp.","OWS overboard valve reported hard to operate – to renew the valve","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","PO no. DEUR200194 for the valve was received and job completed in DD.","2021-03-20T23:59:17","","Completed","2021-03-16T23:59:17","Yes","No","No","Internal"]
[null,null,null,18983,null,"88_27/4/2021 7:31:55 PM","2021-02-15T23:59:17","Breakdown","Ship Staff","Ship Staff Insp.","Two of the cargo tanks COW machine is damaged and removed","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.1","Very High","","","Two new Units recieved at Singapore. New COW units renewed for 1C & 1P COT's.","2021-06-26T23:59:17","DEUR210094","Completed","2021-06-08T23:59:17","No","No","No","Internal"]
[null,null,null,18984,null,"88_27/4/2021 7:24:22 PM","2021-03-27T23:59:17","Defect","Owner / Marine / Tech. Suptd.","Ship Staff Insp.","Stbd Windlass clutch cylinder slight leaking","Deck - Mooring Machinery","Mooring","Equipment Related","9.5","High","","","Windlass vclutch cylinder inspected. refitted after cleaning & inspection. no damage found. function test carried out. No leaks detected.","2021-05-27T23:59:17","","Completed","2021-04-18T23:59:17","No","No","No","Internal"]
[null,null,null,18985,null,"88_27/4/2021 7:28:06 PM","2021-03-27T23:59:17","Defect","Owner / Marine / Tech. Suptd.","Ship Staff Insp.","Aft winch, one of the flange started leaking ","Deck - Mooring Machinery","Mooring","Equipment Related","9.5","High","","","Area around the leak cleaned. upon inspection found damage at the connecting joint. renewed with a spare pipe joint. function testing carried out. no leaks found.","2021-04-20T23:59:17","","Completed","2021-04-07T23:59:17","No","No","No","Internal"]
[null,null,null,18601,null,"88_15/04/2021 15:12:36","2021-04-06T23:59:17","Breakdown","Ship Staff","Ship Staff Insp.","Main air compressor no.1 found LP Piston, LP con rod broken in service. ","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Main air compressor opened up checked for spares, Broken parts LP con rod, LP Piston, Piston rings renewed.","2021-04-15T23:59:17","","Completed","2021-04-12T23:59:17","No","No","No","Internal"]
[null,null,null,18602,null,"88_15/04/2021 14:51:29","2021-04-06T23:59:17","Defect","Ship Staff","Ship Staff Insp.","Main Engine unit no.6, Cylinder oil quill no. 10 pipe cracked and found cylinder oil leaking.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Informed office main engine stopped pipe leakage rectified.","2021-04-08T23:59:17","","Completed","2021-04-07T23:59:17","No","No","No","Internal"]
[null,null,null,18986,null,"88_19-04-2021 16:33:19","2021-04-11T23:59:17","Defect,Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","CO2 room O2 low alarm is active to calibrate and if require spares to order.","Miscellaneous","Safety / LSA / FFA","Equipment Related","5.15","Medium","","","CO2 Room O2 low alarm calibrated found No alarm now.","2021-04-25T23:59:17","","Completed","2021-04-13T23:59:17","No","No","No","Internal"]
[null,null,null,18987,null,"88_19-04-2021 16:28:32","2021-04-12T23:59:17","Observation","Ship Staff","Ship Staff Insp.","HFO Overflow tank level alarm not working.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Transducer renwed now workingl.","2021-04-25T23:59:17","","Completed","2021-04-12T23:59:17","No","No","No","Internal"]
[null,null,null,18988,null,"88_27/04/2021 14:25:48","2021-04-12T23:59:17","Defect","Ship Staff","Ship Staff Insp.","Port HHC jib limit not activated, needs adjustment for proper activation.","Cargo Mach.,Deck - Machinery","Cargo / Ballast Systems","Equipment Related","8.76","Medium","","","Ship's staff to properly re-adjusted limit switch for proper activation, now working satisfactory.","2021-04-25T23:59:17","","Completed","2021-04-23T23:59:17","No","No","No","Internal"]
[null,null,null,18989,null,"88_19-04-2021 16:23:48","2021-04-13T23:59:17","Defect","Ship Staff","Ship Staff Insp.","S/T Lub oil gravity tank has issue with its alarm to trouble shoot and necessary spares to order.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Ships staff checked and rectified the problem.","2021-04-25T23:59:17","","Completed","2021-04-21T23:59:17","No","No","No","Internal"]
[null,null,null,19820,null,"88_21-Jun-21 6:48:13 AM","2021-05-01T23:59:17","Defect","Ship Staff","Ship Staff Insp.","ANEMOMETER NOT WORKING","Navigation - Others","Navigation","Equipment Related","4.7","High","","","ANEMOMETER REPAIRED WITH OLD SPARES, TESTEDV WORKING SATISFACTORY. ( WIND SPEED TRANSMITTER RENEWED)","2021-07-31T23:59:17","DEUR210116","Completed","2021-07-10T23:59:17","No","No","No","Internal"]
[null,null,null,19589,null,"88_24/5/2021 5:47:16 AM","2021-05-14T23:59:17","Defect","Ship Staff","Ship Staff Insp.","defective Pressure sensor for Slop (S) COT.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","Renewal carried out. Pressure sensor zero calibration carried out. Readings compared with Analogue pressure gauge. In good condition","2021-05-18T23:59:17","","Completed","2021-05-15T23:59:17","No","No","No","Internal"]
[null,null,null,19590,null,"88_24/5/2021 5:41:49 AM","2021-05-17T23:59:17","Defect","Ship Staff","Ship Staff Insp.","Fire bilge & ballast pump power & control circuit defective & not working","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","Breaker renewed & Function test carried out. Working satisfactory. Job reported in PAL as unplaned  job No: V-DEUR012870/21.","2021-05-19T23:59:17","","Completed","2021-05-19T23:59:17","No","No","No","Internal"]
[null,null,null,19591,null,"88_30-May-21 4:35:45 PM","2021-05-23T23:59:17","Defect","Ship Staff","Ship Staff Insp.","NO 1 Aux engine lube oil priming pump starter control circuit not working and main contactor chattering.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","No 1 aux engine lube oil priming pump starter control circuit electronic OCR renewed as found not working properly,after replacing Electronic  OCR all found working in good order,aux engine stopped and checked for auto standby start,found circuit working satisfactory.","2021-05-26T23:59:17","","Completed","2021-05-24T23:59:17","No","No","No","Internal"]
[null,null,null,19588,null,"88_31-May-21 4:51:13 PM","2021-05-26T23:59:17","Defect","Ship Staff","Ship Staff Insp.","cargo pump room fan( stbd)  no 1 working with excessive  abnormal noise and vibration .","Elect. Mach. & Equip.","Cargo / Ballast Systems","Equipment Related","","","","","fan assembly to be removed and to check for motor and stuffing box ,bearing found in damaged condition ,bearings renewed.","2021-06-04T23:59:17","DEUR210128   item no 66 ( engine stores)","Completed","2021-06-09T23:59:17","No","No","No","Internal"]
[null,null,null,19818,null,"88_22/6/2021 5:27:25 AM","2021-06-03T23:59:17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Main deck shows the presence of Spot rust & dull appearance.","Miscellaneous","General Appearance","External Factors","11.3","Medium","","","hydroblasting, primering & painting completed.","2021-12-10T23:59:17","","Completed","2021-11-24T23:59:17","No","No","No","Internal","Advise progress on same with every DDRL.. Target date revised."]
[null,null,null,19821,null,"88_22/6/2021 5:06:33 AM","2021-06-03T23:59:17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Main deck stained around cargo manifold areas (P/S)","Miscellaneous","General Appearance","External Factors","11.3","Medium","","","Areas hydroblasted & outfittings chipped/primered. Old Stained paint renewed with new one & New markings carried out.","2021-08-31T23:59:17","","Completed","2021-07-12T23:59:17","No","No","No","Internal","Advise progress on same with every DDRL."]
[null,null,null,19822,null,"88_22/6/2021 5:14:10 AM","2021-06-03T23:59:17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Poor, unsafe life vest given to visitor boarding the vessel through combination ladder.","LSA / FFA","Safety / LSA / FFA","External Factors","5.5","Low","","","New floatation type vests recieved at Galveston, Same marked with vessel name & put in use. 5 numbers in use.","2021-08-27T23:59:17","DEUR 210164","Completed","2021-07-18T23:59:17","No","No","No","Internal","210131 was the store to be supplied in Singapore. What is new RO no for supply in USA."]
[null,null,null,19823,null,"88_22/6/2021 5:21:28 AM","2021-06-03T23:59:17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Accomodation block P & S yellowish","Accommodation","General Appearance","External Factors","11.8","Low","","","spot derusted & painted. Weeping marks washed & cleaned.","2021-09-25T23:59:17","","Completed","2021-09-09T23:59:17","No","No","No","Internal","Advise progress on same with every DDRL. Target date revised."]
[null,null,null,19830,null,"88_22/6/2021 6:02:52 AM","2021-06-03T23:59:17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","IG line to COT 4C appearance of Spot Rust","Deck - Pipe / Fittings","General Appearance","External Factors","11.4","Very High","","","Sporadic rust spots derusted & painted","2021-09-25T23:59:17","","Completed","2021-08-29T23:59:17","No","No","No","Internal","Advise progress on same with every DDRL. Target date revised."]
[null,null,null,19831,null,"88_22/6/2021 6:18:30 AM","2021-06-03T23:59:17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Wheelhouse window frame rusted","Accommodation","General Appearance","External Factors","11.6","Medium","","","spot derusting & painting carried out","2021-08-30T23:59:17","","Completed","2021-07-06T23:59:17","No","No","No","Internal","Advise progress on same with every DDRL."]
[null,null,null,19832,null,"88_22/6/2021 6:07:57 AM","2021-06-03T23:59:17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Emergency Gen room weathertight door packing channel wasted & holed","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","External Factors","11.6","Medium","","","Wasted part fabricated & renewed. Rubber packing renewed. Painting of the channel carried out.","2021-09-02T23:59:17","","Completed","2021-06-28T23:59:17","No","No","No","Internal"]
[null,null,null,19833,null,"88_22/6/2021 6:20:58 AM","2021-06-03T23:59:17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Deck plate aft of FWG Rusted","Miscellaneous","General Appearance","External Factors","11.3","Medium","","","Same  derusted & painted","2021-09-25T23:59:17","","Completed","2021-06-21T23:59:17","No","No","No","Internal","Advise progress on same with every DDRL. target date revised."]
[null,null,null,19834,null,"88_22/6/2021 6:10:58 AM","2021-06-03T23:59:17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","CO2 Room weathertight door lower packing channel rusted","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","External Factors","11.6","Medium","","","Rubber packing removed. Door channel derusted. painted. New Rubber packing renewed.","2021-08-28T23:59:17","","Completed","2021-06-21T23:59:17","No","No","No","Internal"]
[null,null,null,19835,null,"88_22/6/2021 6:13:55 AM","2021-06-03T23:59:17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Accomodation entrance door @ Sunken deck W/T door lower packing channel rusted","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","External Factors","11.6","Medium","","","Rubber packing removed. Door channel derusted. painted. New Rubber packing renewed.","2021-08-27T23:59:17","","Completed","2021-06-21T23:59:17","No","No","No","Internal"]
[null,null,null,19836,null,"88_22/6/2021 6:29:33 AM","2021-06-03T23:59:17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","EGCS deck house emergency escape IMO Symbols not displayed.","LSA / FFA","Safety / LSA / FFA","Human Error","10.15","Low","","","All escape routes marked with IMO Symbols","2021-08-30T23:59:17","","Completed","2021-06-19T23:59:17","No","No","No","Internal"]
[null,null,null,19837,null,"88_22/6/2021 6:38:57 AM","2021-06-03T23:59:17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","EGCS deck house telephone directory next to telephone missing","Documentation","Communication","Human Error","","","","","Area posted with a new Telephone directory list","2021-08-30T23:59:17","","Completed","2021-06-19T23:59:17","No","No","No","Internal"]
[null,null,null,19824,null,"88_29/6/2021 4:55:32 PM","2021-06-05T23:59:17","Defect","Ship Staff","Ship Staff Insp.","Erroneous reading on the Rosemount radar for FPT Sounding. suspected leaks on the Pnuematic air line","Hull & Tanks","Cargo / Ballast Systems","External Factors","2.9","Medium","","","Leak test carried out on the fittings. Air control unit checked for functionality. Defective solenoid valve assembly renewal carried out. Accurate readings obtained","2021-09-02T23:59:17","","Completed","2021-06-26T23:59:17","No","No","No","Internal"]
[null,null,null,19819,null,"88_17/6/2021 12:32:09 PM","2021-06-09T23:59:17","Defect","Ship Staff","Ship Staff Insp.","Missing Stand pipe for venting of ballast tanks atmosphere incase of Oil leakage into the water ballast tanks.","Deck - Pipe / Fittings","Cargo / Ballast Systems","External Factors","","","","","Vessel recieved Consumables at Singapore. Same pipe fabricated & function testing carried out.","2021-10-15T23:59:17","DEUR210175","Completed","2021-09-10T23:59:17","No","No","No","Internal","Stores will be supplied at next port . Target date revised accordingly."]
[null,null,null,19829,null,"88_23-Jun-21 10:14:30 PM","2021-06-09T23:59:17","Defect","Ship Staff","Ship Staff Insp.","IRIDIUM CITADEL PHONE NOT WORKING","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","EXISTING IRIDIUM SYSTEM DE-COMMISSIONED AS PER THE OFFICE MAIL AND IT IS NOT REQUIRED.(With reference to Iridium phone for citadel purpose.\n\nManagement has decided not to supply any new IOP units and accessories for Citadel purpose.\n\nIf units are installed earlier and working, we will continue using.\n\nIf it is faulty then remove the place and no more new installation require.\n\n\n\nPresent unit is in in operational. So remove from the place. When any checklist comes whether vessel is fitted with any CITADEL equipment then answer to say NO.\n\nIf we say YES then we need to follow subsequent criteria.\n\n\n\nSo meanwhile we are not sending any spares for faulty IOP system for Citadel.\n\nKind Regards\n\nKamlesh Solanki\n\nFleet Manager (Electrical / Support)\n\n","2021-06-25T23:59:17","","Completed","2021-06-26T23:59:17","No","No","No","Internal"]
[null,null,null,19825,null,"88_23-Jun-21 10:19:49 PM","2021-06-11T23:59:17","Defect","Ship Staff","Ship Staff Insp.","IG .DECK SEAL PRESSURE SWITCH DEFECTIVE","Inert Gas","Eng. / Strg. Comp.","Equipment Related","","","","","Deck seal pressure switch new installed and tested found all working satisfactory. tested ","2021-08-13T23:59:17","DEUR210148","Completed","2021-07-18T23:59:17","No","No","No","Internal","Spares on order and will be supplied once ready."]
[null,null,null,19826,null,"88_27/06/2021 18:08:44","2021-06-15T23:59:17","Defect","Ship Staff","Ship Staff Insp.","Engine local telegraph unit showing telegraph failure.","E/R - Main Engine,Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","IO card received 3 pcs but renewed with the old one available onboard prior USCG inspection.received 3 cards kept as spare to be changed all 3 cards incase alarm occurs again.","2021-07-25T23:59:17","RO no: DEUR210152","Completed","2021-07-13T23:59:17","No","No","No","Internal","Required PCB will be supplied in USA."]
[null,null,null,19838,null,"88_23-Jun-21 10:29:00 PM","2021-06-17T23:59:17","Defect","Ship Staff","Ship Staff Insp.","Bridge window wiper (STBD) non operational.","Navigation - Others","Navigation","Equipment Related","","","","","stbd window wiper removed from the place,renewed the belt assembly and greasing carried out,after repairs ,wiper tested and found working satisfactory.","2021-06-18T23:59:17","","Completed","2021-06-18T23:59:17","No","No","No","Internal"]
[null,null,null,19827,null,"88_28/06/2021 12:31:24","2021-06-21T23:59:17","Defect","Ship Staff","Ship Staff Insp.","Engage and disengage cluth of Starboard windlass and mooring winch is leaking from seal.","Deck - Machinery","Mooring","Equipment Related","9.2","Very High","","","Clucth assembly received at Singapore on 15th Sept renewed, tested found working satisfactory.","2021-09-20T23:59:17","DEUR210155","Completed","2021-09-15T23:59:17","No","No","No","Internal","Understand spares received and will be attended. Target date revised accordingly."]
[null,null,null,19828,null,"88_28/06/2021 12:27:42","2021-06-22T23:59:17","Defect","Ship Staff","Ship Staff Insp.","Starboard windlass speed is found to be low as compared to makers. Windlass speed supposed to be 3 minutes for 27 metres instead here the speed is 4 minutes 30 seconds for 27 metres.","Deck - Machinery","Mooring","Equipment Related","9.2","Very High","","","Counter balance valve throttle valve opened from 1 turn and also adjusted throttle lever travel to make the same as the Port Side. Speed monitored during lowering while vessel at Vizhinjam.","2021-10-10T23:59:17","","Completed","2021-10-07T23:59:17","No","No","No","Internal","Has this not yet tested ?"]
[null,null,null,20040,null,"88_14-Jul-21 8:03:40 PM","2021-07-09T23:59:17","Defect","Ship Staff","Ship Staff Insp.","NO 2 AUX ENGINE FUEL OIL PRESSURE TRANSMITTER DEFECTIVE AND SHOWING ERRATIC READING.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","PRESSURE TRANSMITTER  REPLACED WITH NEW ONE ,FOUND WORKING IN GOOD ORDER.","2021-07-09T23:59:17","","Completed","2021-07-09T23:59:17","No","No","No","Internal"]
[null,null,null,20041,null,"88_14-Jul-21 7:58:45 PM","2021-07-09T23:59:17","Defect","Ship Staff","Ship Staff Insp.","NO 1 INERT GAS SYSTEM FRESH AIR INTAKE HATCH LIMIT SWITCH DEFECTIVE AND DAMAGED.","Cargo Mach.,Elect. Mach. & Equip.,Inert Gas","Cargo / Ballast Systems","Equipment Related","","","","","NO 1 INERT GAS SYSTEM FRESH AIR INTAKE HATCH LIMIT SWITCH DEFECTIVE AND DAMAGED.SAME REPLACED WITH NEW LIMIT SWITCH ,TESTED AND FOUND WORKING IN GOOD ORDER","2021-07-10T23:59:17","","Completed","2021-07-09T23:59:17","No","No","No","Internal"]
[null,null,null,20387,null,"88_9/8/2021 10:24:41 PM","2021-08-01T23:59:17","Breakdown","Ship Staff","Ship Staff Insp.","Hydroblaster Crankcase showing signs of Oil Contamination & Overflowing from the Oil Cap.","Deck - Machinery","General Appearance","Equipment Related","","","","","Hydroblaster fixed. Investigated the root cause of recurring failure, full report was sent to Technical Dept. through email dated: Mon 18-10-2021 23:58, with subject> RE: DHT Europe - Weekly Work Done Report for 10 Oct - 16 Oct 2021.","2021-10-26T23:59:17","","Completed","2021-10-13T23:59:17","No","No","No","Internal","Spares will be supplied in consultation with maker."]
[null,null,null,20390,null,"88_9/8/2021 10:20:45 PM","2021-08-04T23:59:17","Non Conformity","Ship Staff","Ship Staff Insp.","Duiring Routine inspection of the Lifeboats(P/S) Exhaust pipe it was found to be holed & material worn out. Thickness thinned out.","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.3","Low","","","pipe  taken out of service, new pipe fabrication carried out. same refitted. covered with heat resistant cover, material testing to be carried out. no leaks found","2021-08-11T23:59:17","","Completed","2021-08-09T23:59:17","No","No","No","Internal"]
[null,null,null,20389,null,"88_12/08/2021 15:56:51","2021-08-05T23:59:17","Defect","Ship Staff","Ship Staff Insp.","On 10 August Main engine DGU unit int.error alarm was activated and it was noted that no power supply to the regulator unit. No control from Bridge or ECR and only can control the engine from Local Emergency Manouvering.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Shore technician attended the trouble at Singapore on 15th Sept the trouble rectified changing the IC's and card.Engine tried out found working satisfactory.","2021-09-15T23:59:17","DEUR215117","Completed","2021-09-10T23:59:17","No","No","No","Internal"]
[null,null,null,20391,null,"88_13/08/2021 11:36:48","2021-08-06T23:59:17","Defect","Ship Staff","Ship Staff Insp.","Ballast tank gas detection system was giving trouble as internal leakage analyser pump.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","Fault rectified with vacuum switch ,same system tested and foun working satisfactory.Gas detection system running in auto.","2021-08-25T23:59:17","","Completed","2021-08-08T23:59:17","No","No","No","Internal"]
[null,null,null,20388,null,"88_12/08/2021 15:44:10","2021-08-07T23:59:17","Observation","Ship Staff","Ship Staff Insp.","Oxy/Ace cables is fixed with the gun and spark arresteor using jubilee clips which is to be replaced with the ear clamp.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","5.26","Medium","","","RO raised from office side received at Singapore on 15th Sept and replaced.","2021-09-25T23:59:17","DEUR215119","Completed","2021-09-12T23:59:17","No","No","No","Internal"]
[null,null,null,20791,null,"88_15/09/2021 06:26:36","2021-08-29T23:59:17","Defect","Ship Staff","Ship Staff Insp.","Port provision crane noticed counter balance valve body leakage.","Deck - Machinery","Safety / LSA / FFA","Equipment Related","8.5","Very High","","","Changed with new spare counter balance valve block body and same tried out, working well and fine.","2021-10-10T23:59:17","DEUR215124","Completed","2021-10-10T23:59:17","No","No","No","Internal","Correct spares will be supplied this call Singapore. Target date revised."]
[null,null,null,21296,null,"88_18/9/2021 3:43:21 AM","2021-09-08T23:59:17","Defect","Ship Staff","Ship Staff Insp.","3S WBT Main Valve opening only 80% on the CCR Console Indicator, however locally showing full 100% opened.","Critical Equip.","Cargo / Ballast Systems","Equipment Related","8.8","Medium","","","Valve position indicator renewed, calibrated with local transmitter on deck (3S) \nPresently working satisfactory.","2022-09-25T23:59:17","DEUR210207","Completed","2022-09-10T23:59:17","No","No","No","Internal","Noted."]
[null,null,null,21297,null,"88_18/9/2021 3:15:26 AM","2021-09-10T23:59:17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Damaged tiles in master's bathroom to renew","Accommodation","MLC Related","External Factors","","","","","Vessel recieved new tiles. Same renewed with broken/damaged tiles inside Masters bathroom","2021-12-09T23:59:17","DEUR210211","Completed","2021-10-01T23:59:17","No","No","No","Internal","Noted."]
[null,null,null,21298,null,"88_18/9/2021 3:31:47 AM","2021-09-10T23:59:17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Various manhole of COT (Aft of midship) to derust and paint","Hull & Tanks","General Appearance","External Factors","11.3","Medium","","","Hydroblasted, buffed, primered & final coat painted","2021-12-09T23:59:17","","Completed","2021-11-24T23:59:17","No","No","No","Internal","Noted."]
[null,null,null,21299,null,"88_18/9/2021 3:33:40 AM","2021-09-10T23:59:17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Area below gangway to derust & paint","Deck - Pipe / Fittings","General Appearance","External Factors","11.3","Medium","","","Hydroblasted & painted final coat.","2021-12-09T23:59:17","","Completed","2021-11-20T23:59:17","No","No","No","Internal","Noted."]
[null,null,null,21300,null,"88_27-09-2021 08:23:02","2021-09-10T23:59:17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","BWTS panel near EGB is only bolted at bottom. Few more supports to weld.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Job carried out after taking permission from office. Job completed and closed out.","2021-10-10T23:59:17","","Completed","2021-10-09T23:59:17","No","No","No","Internal","Noted."]
[null,null,null,21301,null,"88_27-09-2021 08:11:57","2021-09-10T23:59:17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Steam leak from ME and DG auto backwash filter steam pipe. To rectify.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Steam leak rectified.","2021-09-25T23:59:17","","Completed","2021-09-19T23:59:17","No","No","No","Internal"]
[null,null,null,21302,null,"88_27-09-2021 08:17:09","2021-09-10T23:59:17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Air duct near by STBD boiler ( 2nd Deck ) is left half painted since yard, Complete the painting.","Miscellaneous","General Appearance","Equipment Related","10.32","Very High","","","Air duct near STBD Boiler ( 2nd deck ) which was left half painted completed paiting.","2021-09-25T23:59:17","","Completed","2021-09-15T23:59:17","No","No","No","Internal"]
[null,null,null,21303,null,"88_27-09-2021 08:34:45","2021-09-10T23:59:17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","EGCS room many garbage laying since docking. To clear.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","EGCS room all garbages removed.","2021-09-15T23:59:17","","Completed","2021-09-15T23:59:17","No","No","No","Internal"]
[null,null,null,21304,null,"88_27-09-2021 08:41:24","2021-09-10T23:59:17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","EGCS room vent operating wheel to derust.","Deck - Pipe / Fittings","General Appearance","Equipment Related","10.29","Medium","","","EGCS room operating wheel de-rusted","2021-09-17T23:59:17","","Completed","2021-09-15T23:59:17","No","No","No","Internal"]
[null,null,null,21305,null,"88_27-09-2021 08:49:48","2021-09-10T23:59:17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Oil leak marks sighted on top of ME crankcase door. To clean and leakage to rectify.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Oil cleaned and leakage rectified.","2021-09-17T23:59:17","","Completed","2021-09-15T23:59:17","No","No","No","Internal"]
[null,null,null,21306,null,"88_27-09-2021 08:53:20","2021-09-10T23:59:17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Sewage shore connection valve on china passage is badly corroded, Valve and bolts to renew.","Deck - Pipe / Fittings","General Appearance","Equipment Related","10.29","Medium","","","Valve and bolts renewed.","2021-09-25T23:59:17","","Completed","2021-09-15T23:59:17","No","No","No","Internal"]
[null,null,null,21307,null,"88_27-09-2021 09:00:17","2021-09-10T23:59:17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Vent heads in china passage to clean and paint.","Deck - Pipe / Fittings","General Appearance","Equipment Related","10.32","Very High","","","Vent head cleaned and painted.","2021-09-20T23:59:17","","Completed","2021-09-18T23:59:17","No","No","No","Internal"]
[null,null,null,21308,null,"88_18/9/2021 3:04:06 AM","2021-09-10T23:59:17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Greasing Points on windlass, winches, watertight doors etc are not highlighted with yellow marking.","Deck - Mooring Machinery","Mooring","Human Error","9.18","Low","","","Marking of all mooring winches, windlass, W/T Doors, Gangways & Cranes carried out","2021-12-09T23:59:17","","Completed","2021-09-23T23:59:17","No","No","No","Internal"]
[null,null,null,21309,null,"88_18/9/2021 3:27:27 AM","2021-09-10T23:59:17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Pilot ladder securing area to derust & paint","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","External Factors","5.47","Medium","","","Port & Stbd Pilot ladder securing outfittings spot derusted, primered & touch up painted","2021-12-09T23:59:17","","Completed","2021-09-23T23:59:17","No","No","No","Internal"]
[null,null,null,21310,null,"88_18/9/2021 3:09:08 AM","2021-09-10T23:59:17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Port side manifold, one of the grating is bent. To Renew","Deck - Pipe / Fittings","General Appearance","External Factors","6.6","Medium","","","Vessel to recieve new fiber gratings. once recieved same to be renewed for port & stbd manifold. Meantime, the bent grating for the port manifold straightened & refixed.","2021-12-09T23:59:17","DEUR215121","Completed","2021-09-15T23:59:17","No","No","No","Internal"]
[null,null,null,21311,null,"88_28/9/2021 10:56:06 PM","2021-09-10T23:59:17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","EGCS Room all doors are very hard to open & operate. To grease.","Miscellaneous","Crew Management","Behaviour Based","","","","","All W/T Doors greasing points greased & freed.","2021-12-09T23:59:17","","Completed","2021-09-20T23:59:17","No","No","No","Internal"]
[null,null,null,21312,null,"88_28/9/2021 11:09:50 PM","2021-09-10T23:59:17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","EGCS room doors and ER entrance from EGCS room doors dog handle not marked with open / close indication.","Miscellaneous","Safety / LSA / FFA","Human Error","","","","","All door Dog handles  marked with open & shut indications","2021-12-09T23:59:17","","Completed","2021-09-20T23:59:17","No","No","No","Internal"]
[null,null,null,21313,null,"88_27-09-2021 08:28:51","2021-09-10T23:59:17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ER Blower plateform ( STBD ) ladder side chain to renew. ","Miscellaneous","General Appearance","Equipment Related","","","","","ER Blower plateform ( STBD ) ladder side chain renewedl. ","2021-09-25T23:59:17","","Completed","2021-09-24T23:59:17","No","No","No","Internal"]
[null,null,null,21314,null,"88_27-09-2021 08:45:37","2021-09-10T23:59:17","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Fish room fan making noise . To overhaul.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Fish room fan noise investigated and rectified.","2021-09-25T23:59:17","","Completed","2021-09-24T23:59:17","No","No","No","Internal"]
[null,null,null,21315,null,"88_27-09-2021 08:56:56","2021-09-10T23:59:17","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Steam leakage from steam trap aft of Aux Boiler.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Steam leak rectified.","2021-09-22T23:59:17","","Completed","2021-09-20T23:59:17","No","No","No","Internal"]
[null,null,null,21587,null,"88_5/10/2021 8:20:29 PM","2021-09-24T23:59:17","Critical Equipment","Ship Staff","Ship Staff Insp.","1P WBT Showing erractic readings. Failure of solenoid Valve","Deck - Pipe / Fittings,Hull & Tanks","Cargo / Ballast Systems","External Factors","","","","","Vessel adjusted valve positioning transmitter locally.","2022-08-25T23:59:17","","Completed","2022-08-27T23:59:17","No","No","No","Internal","Spares not yet ready. Will be arranged at convenient port."]
[null,null,null,21588,null,"88_6/10/2021 4:26:17 PM","2021-09-26T23:59:17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Angle is not marked on angle indicator of both gangway..","Deck - Pipe / Fittings","ISM Related","Human Error","","","","","Vessel marked the Gangway Angle indicator with with angle allowed on the indicator alongwith other zero & intermediate markings","2021-12-27T23:59:17","","Completed","2021-09-30T23:59:17","No","No","No","Internal"]
[null,null,null,21589,null,"88_13/10/2021 8:46:56 AM","2021-09-26T23:59:17","Defect","Ship Staff","Ship Staff Insp.","Main steam valve of the boiler to COPT bonnet gasket leaking.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Bonnet gasket for the Main COPT steam valve renewed.","2021-10-07T23:59:17","","Completed","2021-09-28T23:59:17","No","No","No","Internal"]
[null,null,null,21590,null,"88_13/10/2021 8:41:02 AM","2021-09-26T23:59:17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","The paint of the bulkhead of Sludge holding tank ( near Stbd boiler) is peeled off at many places. To repaint.","Miscellaneous","Eng. / Strg. Comp.","External Factors","10.32","Very High","","","Peeled off paint was removed and painted.","2021-10-08T23:59:17","","Completed","2021-10-07T23:59:17","No","No","No","Internal"]
[null,null,null,21591,null,"88_13/10/2021 8:42:26 AM","2021-09-26T23:59:17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","The cable cover near the stairs of Steering Gear room is removed and kept aside. To fit.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Human Error","10.32","Very High","","","Cover fixed back in place.","2021-10-03T23:59:17","","Completed","2021-10-02T23:59:17","No","No","No","Internal"]
[null,null,null,21592,null,"88_13/10/2021 8:44:40 AM","2021-09-26T23:59:17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Leaking pipe of Sludge transfer on China passage to renew.","Deck - Pipe / Fittings","Eng. / Strg. Comp.","External Factors","10.32","Very High","","","Leaking pipe was removed and wasted area replaced with new pipe. Foxed back and same tried out , found all satisfactory.","2021-10-11T23:59:17","","Completed","2021-10-03T23:59:17","No","No","No","Internal"]
[null,null,null,21593,null,"88_13/10/2021 8:49:27 AM","2021-10-01T23:59:17","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Sludge and sewage line to shore connection valve bolt and nuts to renew and same is corroded and wasted.","Deck - Pipe / Fittings","Eng. / Strg. Comp.","External Factors","10.32","Very High","","","Nuts and bolts removed and same renewed with new.","2021-10-09T23:59:17","","Completed","2021-10-07T23:59:17","No","No","No","Internal"]
[null,null,null,21617,null,"88_19-10-2021 01:05:13","2021-10-12T23:59:17","Non Conformity","Ship Staff","Ship Staff Insp.","Four (4) nos. of Helmet for the Fireman's Outfit are having no Face Shields to protect the smoke divers.","LSA / FFA","Safety / LSA / FFA","Industry Issue","8.65","Low","","","Face shield renewed","2021-10-15T23:59:17","DEUR210230 - FIREMAN SAFETY HELMET WITH CLEAR VISOR","Completed","2021-10-14T23:59:17","No","No","No","Internal"]
[null,null,null,21618,null,"88_19-10-2021 01:10:23","2021-10-12T23:59:17","Observation","Ship Staff","Ship Staff Insp.","Limit switch for Rescue Boat Davit (Lifeboat Port) El Motor High Speed is out of operation.","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.3","Low","","","Limit switch reinstated/connected back into the circuit by ETO.","2021-10-20T23:59:17","","Completed","2021-10-18T23:59:17","No","No","No","Internal"]
[null,null,null,21619,null,"88_19-10-2021 01:16:48","2021-10-12T23:59:17","Defect","Ship Staff","Ship Staff Insp.","Port HHC jib limit activation bracket is corroded, shall be attended on priority basis.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.5","Very High","","","Bracket plate to remove and brought down to Eng Workshop and welded, also Limit switch holding plate was adjusted to fit the said Bracket plate cam arrangement.","2021-10-15T23:59:17","","Completed","2021-10-19T23:59:17","No","No","No","Internal"]
[null,null,null,22529,null,"88_02/11/2021 08:28:15","2021-10-20T23:59:17","Breakdown","Ship Staff","Ship Staff Insp.","No.1 Pump room Fan Coupling for El Motor/Impeller damaged. El motor running when started but observed that the impeller is not turning.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","5.18","High","","","Pump room Vent Fan Unit opened and overhauled. Fixed the couplings, tested function of fan satisfactory and fully functional.","2021-12-10T23:59:17","DEUR210165 - VENTILATION/AIR-COND SYS FOR PUMP ROOMS","Completed","2021-11-15T23:59:17","No","No","No","Internal","Understand fan is fully operational now."]
[null,null,null,22673,null,"88_19-11-2021 09:34:22","2021-11-02T23:59:17","Defect","Ship Staff","Ship Staff Insp.","No.2 ECDIS Showing Alarm generated for Low Battery.","Navigation - ECDIS","Navigation","Equipment Related","4.7","High","","","After troubleshooting assisted by the Maker, it was learned that the cause of the alarm was faulty 24V DC UPS. The maker have guaranteed Service Engineer to attend vessel on the next con port.","2022-03-25T23:59:17","DEUR220012","Completed","2022-03-19T23:59:17","No","No","No","Internal"]
[null,null,null,22675,null,"88_19-11-2021 09:43:52","2021-11-11T23:59:17","Defect","Ship Staff","Ship Staff Insp.","Newly received/installed Anemometer Transmitter faulty. Showing only black display on the indicator panel from both the Bridge and CCR.","Navigation - Others","Navigation","Equipment Related","4.7","High","","","Manage to resolve the issue by using Old PCB still available onboard and by swapping Wind Speed Sensors (mix and matched). Anemometer is  working satisfactory. Once the replacement new PCB from the vendor received onboard - vessel shall keep it as spare.","2021-12-07T23:59:17","DEUR210116 - ANEMOMETER  TRANSMITTER   TYPE: AT-3N","Completed","2021-11-18T23:59:17","No","No","No","Internal","Replacement will be connected in USA."]
[null,null,null,22712,null,"88_01-12-2021 09:32:39","2021-11-23T23:59:17","Defect","Ship Staff","Ship Staff Insp.","I.S. Barrier module (KFDO-CS-EX2.51P) for VECS Pressure Transmitter signal to CCR Panel faulty.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.19","High","","","RECEIVED NEW SPARES AND IS BARRIER RENEWED. TESTED AND FOUND WORKING SATISFACTORY.","2022-04-15T23:59:17","DEUR210232 - VAPOUR MONITORING SYSTEM I.S. BARRIER","Completed","2022-03-17T23:59:17","No","No","No","Internal","Spares will be arranged once ready."]
[null,null,null,23279,null,"88_3/1/2022 7:23:44 am","2021-12-17T23:59:17","Defect","Ship Staff","Ship Staff Insp.","IG Plant Oxygen (O2) content remote display Isolation Amplifier faulty.","Inert Gas","Eng. / Strg. Comp.","Equipment Related","8.19","High","","","Replaced the faulty PR2204 Isolation Amplifier with new spare found extra in the Aux Boilers spare part box.","2022-03-26T23:59:17","","Completed","2022-01-08T23:59:17","No","No","No","Internal"]
[null,null,null,23280,null,"88_3/1/2022 4:58:24 am","2021-12-23T23:59:17","Defect","Ship Staff","Ship Staff Insp.","Mechanical Seal of No.2 SW Feed Pump for EGCS leaking.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Received spare mechanical seal on 19th Mar-2022. Overhauled No.2 SW Feed Pump and renewed mechanical seal.","2022-03-25T23:59:17","DEUR220001","Completed","2022-03-21T23:59:17","No","No","No","Internal"]
[null,null,null,23635,null,"88_12/1/2022 8:36:37 AM","2022-01-06T23:59:17","Critical Equipment","Ship Staff","Ship Staff Insp.","# 1,2 & 5 Foam Monitors found leaking from thevalve gland and flanges","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.35","Medium","","","Overhauling Leaking Foam Monitors is in progress.","2022-03-26T23:59:17","","Completed","2022-03-14T23:59:17","No","No","No","Internal"]
[null,null,null,23636,null,"88_12/1/2022 8:41:19 AM","2022-01-06T23:59:17","Defect","Ship Staff","Ship Staff Insp.","Stbd anchor bow stopper hinge supporting pin is bent","Miscellaneous","Mooring","Equipment Related","9.2","Very High","","","Remove the Pin and shift to Eng Workshop and make necessary repairs.","2022-03-23T23:59:17","","Completed","2022-03-23T23:59:17","No","No","No","Internal"]
[null,null,null,23637,null,"88_12/1/2022 8:54:38 AM","2022-01-06T23:59:17","Defect","Ship Staff","Ship Staff Insp.","Magnetic Compass Glass is opaque at heading location making it hard to read out the compass heading.","Navigation - Others","Navigation","External Factors","4.9","Medium","","","Glass to be turn around so that Mag heading can be read.","2022-03-26T23:59:17","","Completed","2022-03-14T23:59:17","No","No","No","Internal"]
[null,null,null,23638,null,"88_12/1/2022 9:06:11 AM","2022-01-06T23:59:17","Defect","Ship Staff","Ship Staff Insp.","Wind alarm indicator light on deck ( accmdn front) is inoperational.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","4.7","High","","","Need to order new light, RO raised.","2022-04-10T23:59:17","DEUR220023","Completed","2022-03-25T23:59:17","No","No","No","Internal"]
[null,null,null,23639,null,"88_12/1/2022 9:11:17 AM","2022-01-06T23:59:17","Defect","Ship Staff","Ship Staff Insp.","Few Mooring winches Break engage/Disengage Levers found hard to operate.","Deck - Mooring Machinery","Mooring","Human Error","9.14","Medium","","","Need to de-rust and free the levers.","2022-02-05T23:59:17","","Completed","2022-02-03T23:59:17","No","No","No","Internal"]
[null,null,null,23640,null,"88_12/1/2022 10:11:35 AM","2022-01-06T23:59:17","Critical Equipment","Ship Staff","Ship Staff Insp.","Port side Pump room Blower noisy during operation.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.23","Medium","","","No. 2 pump room blower port side overhauled, electrical motor and fan  housing bearing renewed, spider coupling renewed. pump room blower tested found satisfactory.","2022-08-25T23:59:17","","Completed","2022-07-26T23:59:17","No","No","No","Internal","Understand this has been corrected."]
[null,null,null,23765,null,"88_1/2/2022 5:14:40 AM","2022-01-26T23:59:17","Defect","Ship Staff","Ship Staff Insp.","4~5 nos of upper deck external explosion lights safety guard protection grill broken at few places.","Deck - Pipe / Fittings","ISM Related","External Factors","11.11","Very High","","","Need to replace the lights if protective cover grills can not be repaired or fabricated.","2022-03-25T23:59:17","","Completed","2022-02-05T23:59:17","No","No","No","Internal"]
[null,null,null,23766,null,"88_1/2/2022 5:20:32 AM","2022-01-26T23:59:17","Defect","Ship Staff","Ship Staff Insp.","1) Pump Room Flooding dampers operating housing metal box hinge cover broken and overall condition of box is poor condition.\n\n2) Stbd hose handling crane operating box protection cover hinge is broken.","Deck - Pipe / Fittings","Cargo / Ballast Systems","External Factors","","","","","Fabrication of the new box completed, only to complete fitted back the mountings and connection.","2022-03-10T23:59:17","","Completed","2022-02-03T23:59:17","No","No","No","Internal"]
[null,null,null,23767,null,"88_1/2/2022 5:25:20 AM","2022-01-26T23:59:17","Observation","Ship Staff","Ship Staff Insp.","In Scubber tower at few places fire detector IMO symbol isfound missing.","LSA / FFA","Safety / LSA / FFA","Human Error","5.39","Very High","","","Need to post IMO safety symbol at the missing places.","2022-02-10T23:59:17","","Completed","2022-02-02T23:59:17","No","No","No","Internal"]
[null,null,null,23768,null,"88_1/2/2022 5:32:20 AM","2022-01-26T23:59:17","Defect","Ship Staff","Ship Staff Insp.","Gyro # 1& 2 showing heading diff of 0.5~3 deg even after correcting it manually.","Navigation - Others","Navigation","Equipment Related","4.9","Medium","","","Need to seek assistance from Mr. Kamlesh Solanki & Nav Support.","2022-03-26T23:59:17","","Completed","2022-03-14T23:59:17","No","No","No","Internal"]
[null,null,null,23873,null,"88_16/2/2022 9:13:49 AM","2022-02-10T23:59:17","Observation","Ship Staff","Ship Staff Insp.","4 Nos of external lights supports are wasted on poop deck under Srbbuer tower.","Accommodation","ISM Related","External Factors","11.9","Low","","","Need to fabricate new supports in En Workshop and renew the wasted supports.","2022-05-05T23:59:17","","Completed","2022-03-23T23:59:17","No","No","No","Internal"]
[null,null,null,23874,null,"88_17/2/2022 4:38:01 am","2022-02-10T23:59:17","Defect","Ship Staff","Ship Staff Insp.","Release cabinet of fixed CO2 fire fighting system inside the CO2 room both are found having crack iwo securing holes.","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.35","Medium","","","CO2 release cabinet inside CO2 room for pump room and engine room replaced with newly received cabinet. ","2022-06-17T23:59:17","DEUR220059","Completed","2022-05-29T23:59:17","No","No","No","Internal"]
[null,null,null,24156,null,"88_26/2/2022 3:06:02 PM","2022-02-21T23:59:17","Defect","Ship Staff","Ship Staff Insp.","Bridge ME Telegraph Printer Motor belt found broken.","Navigation - Others","Navigation","Equipment Related","4.3","Medium","","","installed the newly received printer & is under observation.","2022-09-25T23:59:17","DEUR225021","Completed","2022-08-31T23:59:17","No","No","No","Internal"]
[null,null,null,24158,null,"88_26/2/2022 10:14:04 AM","2022-02-21T23:59:17","Observation","Ship Staff","Ship Staff Insp.","Emg'y generator room CO2 release operating box cover wasted and securing hook broken. ","Miscellaneous","ISM Related","External Factors","5.35","Medium","","","Bolted securing arrangement fabricated and working satisfactory. ","2022-04-20T23:59:17","","Completed","2022-02-24T23:59:17","No","No","No","Internal"]
[null,null,null,24157,null,"88_3/3/2022 12:55:49 pm","2022-02-24T23:59:17","Defect","Ship Staff","Ship Staff Insp.","EGCS Sea Water Feed Pump Sea Chest - Strainer Bucket/Insert screen mesh wasted away/holed by corrosion. Vessel will require new set of strainer insert for replacement.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","New spare Filter received in Singapore under RO DEUR220002.","2022-04-10T23:59:17","DEUR220002 - EGCS - SW FEED PUMPS FILTER","Completed","2022-03-14T23:59:17","No","No","No","Internal"]
[null,null,null,25150,null,"88_26/4/2022 3:14:10 PM","2022-03-14T23:59:17","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","No1 HFO bunker (S) level gauge box in p/p room hanging loose – to secure adequately. ","Miscellaneous","ISM Related","Equipment Related","","","","","No 1 HFO bunker ( S) level gauge box in p/p room adequately secured.","2022-06-13T23:59:17","","Completed","2022-04-07T23:59:17","No","No","No","Internal"]
[null,null,null,25151,null,"88_26/4/2022 3:28:46 PM","2022-03-14T23:59:17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","EGCS deck house louvre to derust & paint","Miscellaneous","Eng. / Strg. Comp.","External Factors","","","","","EGCS deck house louvre derusted and painted","2022-06-13T23:59:17","","Completed","2022-04-06T23:59:17","No","No","No","Internal"]
[null,null,null,25152,null,"88_26/4/2022 3:36:30 PM","2022-03-14T23:59:17","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","EGCS electrical panels in EGCS tower – to install Air Con. ","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","EGCS electrical panels in EGCS tower – Air con installed.","2022-06-13T23:59:17","","Completed","2022-04-07T23:59:17","No","No","No","Internal"]
[null,null,null,25153,null,"88_26/4/2022 3:39:54 PM","2022-03-14T23:59:17","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Incinerator sludge p/p inlet side short pipe section soft repaired, renew defective pipe. ","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Inappropriate Procedure","","","","","Incinerator sludge p/p inlet side short pipe section soft repaired- defective pipe renewed.","2022-06-13T23:59:17","","Completed","2022-04-04T23:59:17","No","No","No","Internal"]
[null,null,null,25154,null,"88_26/4/2022 3:46:34 PM","2022-03-14T23:59:17","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","IGG sea water line filter cover has salt deposit, renew gasket. ","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","IGG sea water line filter cover has salt deposit, gasket renewed.","2022-06-13T23:59:17","","Completed","2022-03-28T23:59:17","No","No","No","Internal"]
[null,null,null,25157,null,"88_26/4/2022 3:30:48 PM","2022-03-14T23:59:17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","EGCS jet section upper inlet pipe v/v inlet flange minor leakage – renew gasket. ","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","EGCS jet section upper inlet pipe v/v inlet flange minor leakage – Gasket renewed.","2022-06-13T23:59:17","","Completed","2022-04-04T23:59:17","No","No","No","Internal"]
[null,null,null,24921,null,"88_16/4/2022 9:33:43 AM","2022-03-14T23:59:17","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Bosun Store anchor wash line (S) holed, renew wasted pipe section. ","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","Equipment Related","9.2","Very High","","","Vessel need to shift wasted pipe section to workshow and need to renew","2022-06-13T23:59:17","","Completed","2022-06-11T23:59:17","No","No","No","Internal"]
[null,null,null,24922,null,"88_31/3/2022 6:05:47 PM","2022-03-14T23:59:17","Critical Equipment","Ship Staff","Ship Staff Insp.","Following points noticed by ODME service engineer during annual servicing - 1.Cooling Fan ( Old type with rectifier) in OCM unit not running.2. OCM unit pilot lamp 6.3V need to replace.","Critical Equip.","MARPOL Related","Equipment Related","6.13","Low","","","Vessel have replace cooling fan and OCM unit pilot lamp 6.3V on the ODME panel","2022-07-05T23:59:17","DEUR220143","Completed","2022-06-30T23:59:17","No","No","No","Internal"]
[null,null,null,24923,null,"88_31/3/2022 9:05:31 pm","2022-03-16T23:59:17","Breakdown","Ship Staff","Ship Staff Insp.","Main Engine No.2 Aux Blower Impeller catastrophic failure/damaged due to El motor base frame fissure (cracked) leading to bent motor shaft and burnt windings.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Renewed No.2 Aux Blower complete assembly including El Motor and new Impeller.","2022-06-25T23:59:17","DEUR220087 - ME AUX BLOWER IMPELLER","Completed","2022-03-17T23:59:17","No","No","No","Internal"]
[null,null,null,24924,null,"88_16/4/2022 10:19:31 AM","2022-04-01T23:59:17","Defect","Ship Staff","Ship Staff Insp.","Cargo Monitoring System (SAAB) Main Unit Local Display no signal coming from the system. Suspecting DVI to VGA adapter faulty.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.15","High","","","Service engineer attended in Singapore, Required spares renewed. Tried out working satisfactory. ( Monitor renewed, cable adapter renewed)","2022-08-26T23:59:17","","Completed","2022-08-28T23:59:17","No","No","No","Internal"]
[null,null,null,24925,null,"88_16/4/2022 9:26:27 AM","2022-04-08T23:59:17","Defect","Ship Staff","Ship Staff Insp.","Cargo Eductor discharge pressure transmitter (Press./Pneu.) from Pumproom showing zero pressure.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.8","Medium","","","Cargo Eductor  Suction and discharge pressure transmitters in  pump room overhauled and calibrated, working satisfactory.","2022-07-02T23:59:17","","Completed","2022-06-11T23:59:17","No","No","No","Internal"]
[null,null,null,24926,null,"88_16/4/2022 10:04:59 AM","2022-04-09T23:59:17","Breakdown,Defect","Ship Staff","Ship Staff Insp.","Steering Gear Exhaust Fan El Motor winding showing zero resistance (Low Insulation).","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","steering gear fan motor renewed with new spare motor. fan tried out. found working satisfactorily.","2022-05-31T23:59:17","DEUR220097","Completed","2022-05-15T23:59:17","No","No","No","Internal"]
[null,null,null,24927,null,"88_16/4/2022 7:13:20 PM","2022-04-10T23:59:17","Defect","Ship Staff","Ship Staff Insp.","CO2 release cabinet for Emg'y generator on poop deck need fabrication as condition is poor and wasted.","Miscellaneous","ISM Related","External Factors","5.4","High","","","Emergency Generator Room CO2 system, new valve cabinet Fabricated and installed in place.  ","2022-06-10T23:59:17","","Completed","2022-05-29T23:59:17","No","No","No","Internal"]
[null,null,null,25149,null,"88_26/4/2022 4:26:38 PM","2022-04-16T23:59:17","Observation","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","SOPEP eqpt, one bucket in cracked condition approx 10 cm in length. Further ,the buckets provided were of light duty types instead of heavy duty types as stated on the eqpt inventory.","Miscellaneous","MARPOL Related","Human Error","6.1","Medium","","","Cracked bucket replaced with new bucket. Awaiting RO DEUR22012","2022-07-15T23:59:17","DEUR22012","Completed","2022-04-25T23:59:17","No","No","No","External"]
[null,null,null,25155,null,"88_26/4/2022 4:33:28 PM","2022-04-16T23:59:17","Observation","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","There was no H2 span gas available on board to carry out the calibration for the BWTS gas detector. The PMS required 3M calibration to be conducted, however entries made since 01 July 2021 stated calibration was not carried out due to the unavailablity of the span gas onboard.","Cargo Mach.","Cargo / Ballast Systems","External Factors,Human Error","6.22","Medium","","","Shore technician attended the vessel at Tg Bruas for H2 sensor span calibration. All 3 nos of H2 sensors were calibrated satisfactorily and one H2 span gas bottle was delivered to vessel for 3 monthy calibration onboard as per PMS.","2022-07-15T23:59:17","","Completed","2022-04-18T23:59:17","No","No","No","External"]
[null,null,null,25156,null,"88_26/4/2022 4:39:47 PM","2022-04-16T23:59:17","Defect","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","Two Ex prrof type light located outside the Battery room vicinity on E deck stbd/side on the aft side of the external block were noted with water moisture inside the glass cover casings.","Elect. Mach. & Equip.","ISM Related","Equipment Related,External Factors","11.11","Very High","","","Two defective Ex type lights removed and new lights have been installed.","2022-07-15T23:59:17","","Completed","2022-04-21T23:59:17","No","No","No","External"]
[null,null,null,25493,16361,"88_Sun May 01 2022 14:51:30 GMT+0800","2022-04-26T23:59:17","Defect","Others (Eg. Insurance etc.)","Others (Eg. Insurance etc.)","Port and Stbd Anchor Hydraulic brake cylinder oil seal leaking.","Deck - Mooring Machinery","Mooring","Equipment Related","9.20","Medium","","","Port Side Anchor Hydraulic brake cylinder's fully overhauled- shaft, all the seals & bearings are renewed.\nStbd side on Top Cover's- all the seals are renewed. \nAfter renewal of above, both side brakes tested no leakage found & working satisfactory.","2022-08-26T23:59:17","DEUR220112","Completed","2022-09-03T23:59:17","No","No","No","External"]
[null,null,null,25495,99838,"88_Sun May 01 2022 15:21:02 GMT+0800","2022-04-26T23:59:17","Defect","Others (Eg. Insurance etc.)","Others (Eg. Insurance etc.)","Soft patch discovered on Foam line near port side main deck near pump room.","LSA / FFA","Safety / LSA / FFA","Inappropriate Procedure","5.35","Medium","","","Foam line (flange to flange, 1.5 mtrs) to be opened and taken down to engine room workshop for permanent repairs.","2022-05-26T23:59:17","","Completed","2022-04-30T23:59:17","No","No","No","External"]
[null,null,null,25494,73120,"88_Mon May 30 2022 14:55:15 GMT+0800","2022-05-25T23:59:17","Defect","Ship Staff","Ship Staff Insp.","Both Port & Stbd Windlass , anchor lowering speed is very slow.","Deck - Mooring Machinery","Mooring","Equipment Related","9.24","Medium","","","port and stbd windlass anchor lowering and heaving speed checked. counter balance and throttle valve adjusted by Ship staff and technician at singapore. The lowering speed from the makers states that no further adjustment is required.","2022-08-25T23:59:17","","Completed","2022-06-19T23:59:17","No","No","No","Internal"]
[null,null,null,25496,83396,"88_Tue May 31 2022 15:51:44 GMT+0800","2022-05-25T23:59:17","Observation","Ship Staff","Ship Staff Insp.","E/R sludge transfer line to shore connection found corroded and wasted on stbd side near Sludge manifold approximately 2m in length.","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","External Factors","","","","","New pipe fabricated and fitted in place. pipe line tested. all found normal.....","2022-06-25T23:59:17","","Completed","2022-05-27T23:59:17","No","No","No","Internal"]
[null,null,null,25767,31573,"88_Sun Jun 19 2022 10:24:40 GMT+0800","2022-06-09T23:59:17","Breakdown","Ship Staff","Ship Staff Insp.","Aux engine viscosity controller motor found burnt.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","Aux engine viscosity controller motor  received and replaced with ME viscometer and ME viscometer el motor overhauled and fitted to Aux engine viscometer. Presently both viscometers are working satisfactory.","2022-09-25T23:59:17","DEUR 220132","Completed","2022-09-03T23:59:17","No","No","No","Internal"]
[null,null,null,25764,59910,"88_Thu Jun 16 2022 10:35:10 GMT+0800","2022-06-11T23:59:17","Defect","Ship Staff","Ship Staff Insp.","After Mooring Operation at China, Port windlass + Aft spring (Stbd) + Aft breast (Port) hydraulic oil leaking from the high speed lever","Deck - Mooring Machinery","Mooring","Equipment Related","9.14","Medium","","","High speed lever O rings renewed from the Mooring Winches.\nFunction test carried out, all found satisfactory","2022-09-11T23:59:17","","Completed","2022-07-02T23:59:17","No","No","No","Internal","Does vessel have required seals for renewal?"]
[null,null,null,25765,81742,"88_Thu Jun 16 2022 10:40:08 GMT+0800","2022-06-11T23:59:17","Defect","Ship Staff","Ship Staff Insp.","Fixed gas detection system - Ballast showing fault alarm continuously ie  Analyse pump or internal leakage","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","5.21","Medium","","","Vacuum switch calibrated. \nAll ballast tanks sample lines filters cleaned.","2022-09-11T23:59:17","","Completed","2022-07-14T23:59:17","No","No","No","Internal"]
[null,null,null,25766,66582,"88_Sun Jun 19 2022 10:20:18 GMT+0800","2022-06-13T23:59:17","Defect","Ship Staff","Ship Staff Insp.","E/R sludge transfer line to shore connection found corroded and wasted on port side near Sludge manifold approximately 2m in length.","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","External Factors","","","","","New pipe fabricated and boxed back.","2022-08-26T23:59:17","","Completed","2022-06-15T23:59:17","No","No","No","Internal"]
[null,null,null,23634,null,"88_12/1/2022 8:48:29 AM","2022-06-18T23:59:17","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Both Hose handling crane working platform grating corroded and on poor condition and found supported by the band it tape. No securing clips provided","Cargo Mach.","ISM Related","External Factors","8.5","Very High","","","Hose Handling working platform grating renewed with the securing clamps.\nGrating painted with 2 primer + 1 top coat.","2022-09-18T23:59:17","","Completed","2022-07-01T23:59:17","No","No","No","Internal"]
[null,null,null,26081,23232,"88_Tue Jul 05 2022 14:49:22 GMT+0800","2022-06-18T23:59:17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","No 3 DG preheater valve wheel missing.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Wheel fixed from old valve, now operational.","2022-09-18T23:59:17","","Completed","2022-06-30T23:59:17","No","No","No","Internal"]
[null,null,null,26082,32437,"88_Tue Jul 05 2022 14:50:52 GMT+0800","2022-06-18T23:59:17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","No 1 LT cooler one of the press gauge is missing.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Cooler Pressure glass replaced with new one.","2022-09-18T23:59:17","","Completed","2022-06-27T23:59:17","No","No","No","Internal"]
[null,null,null,26083,72337,"88_Tue Jul 05 2022 14:53:01 GMT+0800","2022-06-18T23:59:17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Oil traces found in pump room near one of the cargo vale. Same needs to be investigated and rectified.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.51","Low","","","Air Vent plug for the Remote Hydraulic was Tightened and function test carried out.","2022-09-18T23:59:17","","Completed","2022-07-23T23:59:17","No","No","No","Internal"]
[null,null,null,26084,53644,"88_Tue Jul 05 2022 14:55:32 GMT+0800","2022-06-18T23:59:17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Elevator door chain was found very slack, same need to be adjusted.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.31","Very High","","","New motor installed and chain tightness adjusted. Tried out working satisfactory.","2022-09-18T23:59:17","","Completed","2022-08-30T23:59:17","No","No","No","Internal"]
[null,null,null,26085,84222,"88_Tue Jul 05 2022 14:58:01 GMT+0800","2022-06-18T23:59:17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ER second deck Stbd side area nearby the 16k / 10k steam to be arranged.","Miscellaneous","Eng. / Strg. Comp.","Behaviour Based","11.1","High","","","Area cleaned and arranged. all loose items secured.","2022-09-18T23:59:17","","Completed","2022-06-29T23:59:17","No","No","No","Internal"]
[null,null,null,26077,28277,"88_Sun Jul 03 2022 11:55:53 GMT+0800","2022-06-28T23:59:17","Observation","Ship Staff","Ship Staff Insp.","IG PRESSURE SHOWING DIFFERENCE IN IG PANEL IN CCR AND BRIDGE WHEN COMPARED TO SAAB GUAGE","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.13","Medium","",""," IG LINE PRESSURE TRANSMITTER REPLACED WITH NEW CALIBERATED TRANSMITTER, TRIED OUT WORKING SATISFACTORY.","2022-11-28T23:59:17","","Completed","2022-11-13T23:59:17","No","No","No","Internal"]
[null,null,null,26078,75781,"88_Sun Jul 03 2022 12:30:07 GMT+0800","2022-06-28T23:59:17","Observation","Ship Staff","Ship Staff Insp.","Main Engine Bridge unit - Auto chief panel showing \"Internal Failure\" + \"Telegraph Failure\" alarm at a certain period of time","Navigation - Others","Navigation","Equipment Related","4.7","High","","","The communication cable from the local maneuvering platform's telegraph panel renewed.\nnow no more alarm indication  on the main engine bridge unit & is working satisfactory.","2022-09-28T23:59:17","","Completed","2022-09-02T23:59:17","No","No","No","Internal"]
[null,null,null,26080,42975,"88_Sun Jul 03 2022 15:04:41 GMT+0800","2022-06-28T23:59:17","Observation","Ship Staff","Ship Staff Insp.","Oil drop Leaking from No: 3 COP Casing","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.11","Medium","","","COP #3 casing removed and welded by shore welders in ER workshop.  Casing boxed back.","2022-11-28T23:59:17","","Completed","2022-11-07T23:59:17","No","No","No","Internal"]
[null,null,null,26319,77612,"0_Tue Jul 19 2022 21:06:58 GMT+0800","2022-07-14T23:59:17","Non Conformity","Ship Staff","Ship Staff Insp.","1.\tWhen command from bridge given by steering wheel “Midship”, Bridge and Rudder angle indicator are showing “0” value.\n2.\tWhen command from bridge given by steering wheel “10 degree” PS or Stbd, Bridge and Rudder angle indicator are showing “11 degree” value PS and Stbd.\n3.\tWhen command from bridge given by steering wheel “20 degree” PS or Stbd, Bridge and Rudder angle indicator are showing “22 degree” value PS and Stbd.\n4.\tWhen command from bridge given by steering wheel “30 degree” PS or Stbd, Bridge and Rudder angle indicator are showing “33 degree” value PS and Stbd.\n","Navigation - Others","Navigation","Equipment Related","4.7","High","","","Technicians from steering gear maker and Auto Pilot attended. No 1 Torque motor replaced.","2022-10-12T23:59:17","","Completed","2022-11-04T23:59:17","No","No","No","Internal"]
[null,null,null,26320,53075,"0_Tue Jul 19 2022 21:12:31 GMT+0800","2022-07-14T23:59:17","Defect","Ship Staff","Ship Staff Insp.","Several links between the gypsy and hawse pipe on the starboard anchor have the stud loose. ","Deck - Mooring Machinery","Mooring","Equipment Related","9.20","Medium","","","All the loose studs between gypsy & hawse pipe for both (Port & Stbd) Anchor cables fabricated & repaired after office concurrence.","2022-10-12T23:59:17","","Completed","2022-09-17T23:59:17","No","No","No","Internal"]
[null,null,null,26321,19275,"0_Tue Jul 19 2022 21:19:03 GMT+0800","2022-07-14T23:59:17","Observation","Ship Staff","Ship Staff Insp.","Alarm lights for steering system located on bridge console do not flicker and many alarm lights light up together including Telephone alarm. Isolating system valve close light does not light up","Elect. Mach. & Equip.","Navigation","Equipment Related","","","","","CHECKED AND RECTIFIED.","2022-10-12T23:59:17","","Completed","2022-07-31T23:59:17","No","No","No","Internal"]
[null,null,null,26322,96942,"0_Tue Jul 19 2022 21:31:19 GMT+0800","2022-07-14T23:59:17","Observation","Ship Staff","Ship Staff Insp.","None of the  clothes dryers on board is working","Accommodation","MLC Related","Equipment Related","11.16","Low","","","RENEWED THE BELTS , RECEIVED IN SINGAPORE. TRIED OUT , WORKING SATISFACTORY.","2022-08-26T23:59:17","DEUR220146","Completed","2022-09-01T23:59:17","No","No","No","Internal"]
[null,null,null,26323,79634,"0_Tue Jul 19 2022 21:51:37 GMT+0800","2022-07-14T23:59:17","Observation","Ship Staff","Ship Staff Insp.","Cancel limitation button has to be activated on the Auto Chief Panel during bridge control of ME id RPM has to be increased above 33.","E/R - Main Engine","Emgcy. Systems","Equipment Related","10.20","High","","","Cancel limit button has to be activated from bridge only during maneuvering sudden increase of rpm is required. During normal running scavenge air limiter getting activated and rpm increasing as per load program.","2022-10-12T23:59:17","","Completed","2022-07-25T23:59:17","No","No","No","Internal"]
[null,null,null,26325,57479,"0_Tue Jul 19 2022 21:45:32 GMT+0800","2022-07-14T23:59:17","Observation","Ship Staff","Ship Staff Insp.","Both ECDIS hanging at Times. The EBL control is erratic.","Navigation - ECDIS","Navigation","Equipment Related","4.7","High","",""," SERVICE CARRIED OUT. WORKING SATISFACTORILY","2022-08-26T23:59:17","","Completed","2022-08-29T23:59:17","No","No","No","Internal"]
[null,null,null,26592,32421,"88_Wed Aug 17 2022 23:47:37 GMT+0800","2022-08-10T23:59:17","Defect","Ship Staff","Ship Staff Insp.","No 2 Center Saab gauge not working","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.16","Very High","","","Service engineer attended in Singapore. Fault rectified, working satisfactory.","2022-10-13T23:59:17","","Completed","2022-08-28T23:59:17","No","No","No","Internal"]
[null,null,null,26593,79505,"88_Wed Aug 17 2022 23:53:42 GMT+0800","2022-08-10T23:59:17","Critical Equipment,Non Conformity","Ship Staff","Ship Staff Insp.","No 2 steering motor does not work immediately when  put off for long hours.","Critical Equip.,Navigation - Others","Eng. / Strg. Comp.","Equipment Related","10.39","High","","","Technician from Swift Electronics rectified settings and replaced no 1 Torque motor. All steering motors working well.\nSteering gear technician from Mitsubishi carried out health check up of the steering gear.","2022-09-26T23:59:17","","Completed","2022-11-04T23:59:17","No","No","No","Internal"]
[null,null,null,26761,90671,"88_Wed Aug 24 2022 08:35:26 GMT+0800","2022-08-20T23:59:17","Defect","Ship Staff","Ship Staff Insp.","OBT Level transmitter out of order. Requisition No DEUR220170 has been raised","Hull & Tanks","Eng. / Strg. Comp.","Equipment Related","10.30","High","","","OBT level transmitter renewed, tried out working satisfactory.","2022-11-20T23:59:17","DEUR220170","Completed","2022-11-14T23:59:17","No","No","No","Internal"]
[null,null,null,26766,78889,"88_Thu Aug 25 2022 16:07:54 GMT+0800","2022-08-21T23:59:17","Observation","Ship Staff","Ship Staff Insp.","Stripping pump stroke indicator showing always zero in CCR during pump operational","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.8","Medium","","","Air valve for stroke transmitter overhauled, boxed back, tried out, found OK.","2022-11-21T23:59:17","","Completed","2022-08-27T23:59:17","No","No","No","Internal"]
[null,null,null,26764,12232,"88_Fri Aug 26 2022 08:03:49 GMT+0800","2022-08-22T23:59:17","Defect","Ship Staff","Ship Staff Insp.","When the General alarm switch is pressed in the CCR, Foam room and ECR, the Ships horn does not sound . However the internal speaker system alarm is generated.","LSA / FFA","Communication","Equipment Related","5.14","Very High","","","Requisition DEUR220206 GENERAL EMERGENCY ALARM PUSH BUTTON SWITCH raised. The ships horn does not have to ring.","2022-11-22T23:59:17","","Completed","2022-10-30T23:59:17","No","No","No","Internal"]
[null,null,null,26818,25522,"88_Wed Sep 14 2022 18:37:18 GMT+0800","2022-09-06T23:59:17","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","LO heater steam line leak to rectify.","E/R - Purifier","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","LO Purifier steam outlet line gasket renewed. Tried out, no leak observed.","2022-10-28T23:59:17","","Completed","2022-09-19T23:59:17","No","No","No","Internal","When do you plan to attend?"]
[null,null,null,26819,62336,"88_Wed Sep 14 2022 18:40:34 GMT+0800","2022-09-06T23:59:17","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ME FO heater steam line leak to rectify.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","ME FO heater end cover steam gasket renewed, tried out working satisfactory.","2022-10-05T23:59:17","","Completed","2022-09-18T23:59:17","No","No","No","Internal"]
[null,null,null,26820,35017,"88_Wed Sep 14 2022 20:10:51 GMT+0800","2022-09-06T23:59:17","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Leak source from cargo valve actuator to identify and repair.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","6.4","High","","","Hydraulic valve's air vent valve from inlet side was leaking from thread . Same was replaced & leak stopped. After renewal valve operation carried out for closing & opening found working satisfactory & no sign of any leak .\nRequisition for spare has been raised ","2022-09-27T23:59:17","DEUR220174-VALVE HYDRAULIC SPARES","Completed","2022-09-14T23:59:17","No","No","No","Internal"]
[null,null,null,26821,98562,"88_Wed Sep 14 2022 20:18:25 GMT+0800","2022-09-06T23:59:17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Deck area below cable trays to paint.","Deck - Pipe / Fittings","","External Factors","","","","","All rust stain are removed from Areas below cable trays & painted with green paint ","2022-10-01T23:59:17","","Completed","2022-09-15T23:59:17","No","No","No","Internal"]
[null,null,null,26822,59768,"0_Wed Sep 14 2022 20:22:14 GMT+0800","2022-09-06T23:59:17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","At various locations blue paint used as top coat. To use proper paint.","Miscellaneous","","Human Error","","","","","All blue paint patches on main deck area are painted with green paint as top coat. ","2022-09-27T23:59:17","","Completed","2022-09-26T23:59:17","No","No","No","Internal"]
[null,null,null,26823,83064,"0_Wed Sep 14 2022 20:32:44 GMT+0800","2022-09-06T23:59:17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Two steps of stairs to monkey island is corroded. To renew\t\t\t","Accommodation","General Appearance","External Factors","12.9","High","","","Wasted steps of stairs to monkey island are fabricated & repaired after received concurrence from office.","2022-12-11T23:59:17","","Completed","2022-09-17T23:59:17","No","No","No","Internal"]
[null,null,null,26824,16890,"88_Wed Sep 14 2022 18:51:52 GMT+0800","2022-09-06T23:59:17","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Various drawer in workshop can not close. To rectify ","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Various drawer in workshop sluggish movement rectified.  ","2022-09-15T23:59:17","","Completed","2022-09-12T23:59:17","No","No","No","Internal"]
[null,null,null,26825,70256,"88_Wed Sep 14 2022 18:45:25 GMT+0800","2022-09-06T23:59:17","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Steam leak from AE LO storage tank steam return line.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","AE LO storage tank steam return line gasket renewed. No leaks observed.","2022-10-05T23:59:17","","Completed","2022-09-12T23:59:17","No","No","No","Internal"]
[null,null,null,27571,43288,"88_Fri Nov 11 2022 11:43:24 GMT+0800","2022-09-15T23:59:17","Defect","Ship Staff","Ship Staff Insp.","AE#1 attached jacket water pump leaking from the mechanical seal.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","AE#1 attached jacket water pump overhauled. Mech seal, O-rings and bearings renewed. Pump tried out working satisfactory.\n","2022-10-15T23:59:17","","Completed","2022-09-16T23:59:17","No","No","No","Internal"]
[null,null,null,27573,86506,"88_Fri Nov 11 2022 11:56:02 GMT+0800","2022-09-17T23:59:17","Defect","Ship Staff","Ship Staff Insp.","ME FO Viscometer leaking from mech seal\n","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","ME FO Viscometer overhauled. Mechanical seal, O-rings and bearings renewed. Tried out working satisfactory, no leaks observed.\n","2022-10-07T23:59:17","","Completed","2022-09-19T23:59:17","No","No","No","Internal"]
[null,null,null,27572,72354,"88_Fri Nov 11 2022 11:59:34 GMT+0800","2022-10-12T23:59:17","Defect","Ship Staff","Ship Staff Insp.","Main CSW pump #1 leaking from mechanical seal.\n","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Main CSW pump #1 overhauled. Sleeve, mechanical seal, gaskets and o -rings renewed. Line bearing and casing rings found in good condition. Pump tried out, working satisfactory.\n","2022-10-16T23:59:17","","Completed","2022-10-13T23:59:17","No","No","No","Internal"]
[null,null,null,27570,43125,"88_Fri Nov 11 2022 12:02:52 GMT+0800","2022-10-23T23:59:17","Defect","Ship Staff","Ship Staff Insp.","Boiler uptake pipeline distance piece above Scrubber found heavily corroded and wasted. \n","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","\nBoiler uptake pipeline stub piece above Scrubber replaced with prefabricated one received in Singapore.","2022-11-20T23:59:17","","Completed","2022-11-08T23:59:17","No","No","No","Internal"]
[null,null,null,27747,59090,"88_Tue Nov 29 2022 11:42:21 GMT+0800","2022-11-05T23:59:17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Working platform to fix between DG 1 & 2","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.27","Medium","","","Platform fitted","2022-11-12T23:59:17","","Completed","2022-11-12T23:59:17","No","No","No","Internal"]
[null,null,null,27748,19876,"88_Tue Nov 29 2022 12:08:42 GMT+0800","2022-11-05T23:59:17","Defect,Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Mooring winch gear case oil not clearly visible for few winches","Deck - Mooring Machinery","Mooring","Equipment Related","9.14","Medium","","","Gear case oil removed. Glass cleaned and oil replaced after filtering.","2022-12-29T23:59:17","","Completed","2022-11-14T23:59:17","No","No","No","Internal"]
[null,null,null,27749,56211,"88_Tue Nov 29 2022 12:12:43 GMT+0800","2022-11-05T23:59:17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","AUX Engine No 1 Pre Lub Oil Pump found leaking","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Leak recitified","2022-11-20T23:59:17","","Completed","2022-11-14T23:59:17","No","No","No","Internal"]
[null,null,null,null,40204,"88_Tue Nov 29 2022 12:16:54 GMT+0800","2022-11-05T08:00:00","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","No flow was notified in the transparent hose for the sewage plant","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","All chambers cleaned and flushed. Hoses removed and cleaned. Working satisfactory.","2022-11-12T08:00:00","","Completed","2022-11-12T08:00:00","No","No","No","Internal"]
[null,null,null,27751,43712,"88_Tue Nov 29 2022 12:19:48 GMT+0800","2022-11-05T23:59:17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Cable tray wasted near the Starboard gangway area","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","External Factors","5.47","Medium","","","Cold repair carried out","2022-12-05T23:59:17","","Completed","2022-11-12T23:59:17","No","No","No","Internal"]
[null,null,null,27752,36218,"88_Tue Nov 29 2022 11:45:30 GMT+0800","2022-11-05T23:59:17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ME air cooler (A) manometer reading not clear","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","ME air cooler manometer cleaned and water replenished.","2022-12-11T23:59:17","","Completed","2022-11-18T23:59:17","No","No","No","Internal"]
[null,null,null,27753,54910,"88_Tue Nov 29 2022 12:05:37 GMT+0800","2022-11-05T23:59:17","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","International shore coupling laying loosely in the CO2 room. This needs to be properly secure","LSA / FFA","Safety / LSA / FFA","Human Error","5.37","Low","","","This was not a International shore coupling. It was a fitting made on board with a nakajima coupling on one side and a 8 inch flange on the other side.","2022-11-08T23:59:17","","Completed","2022-11-08T23:59:17","No","No","No","Internal"]
[null,null,null,27754,75829,"88_Tue Nov 29 2022 11:39:34 GMT+0800","2022-11-05T23:59:17","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","LT cooler (S) sea water outlet pressure gauge connection leaking","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","LT cooler (S) sea water outlet pressure gauge connection renewed. Tried out no leak observed.","2023-01-05T23:59:17","","Completed","2022-11-18T23:59:17","No","No","No","Internal"]
[null,null,null,null,90422,"88_Wed Nov 30 2022 20:36:10 GMT+0800","2022-11-15T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Aux boiler # 1 Atomizing steam controller having sluggish movement.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Aux boiler # 1 Atomizing steam controller replaced with new one. Tried out working satisfactory. PCB card failure.","2022-11-29T08:00:00","","Completed","2022-11-16T08:00:00","No","No","No","Internal"]
[null,null,null,null,72489,"0_Sun Jul 03 2022 12:00:51 GMT+0800","2022-06-18T08:00:00","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Two ovens in galley one coil not working. One Oven in galley disconnected from power .","Accommodation","MLC Related","Equipment Related","11.13","Low","","","Found coils damaged , requisition raised for the same RO No. DEUR220157","2022-11-28T08:00:00","DEUR220157","Completed","2022-12-08T08:00:00","No","No","No","Internal"]
[null,null,null,null,38982,"88_Thu Dec 01 2022 11:33:38 GMT+0800","2022-11-24T08:00:00","Defect","Ship Staff","Ship Staff Insp.","EGCS SW feed pump #1 discharge line stub piece leaking.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","EGCS SW feed pump #1 discharge line stub piece renewed.","2022-12-30T08:00:00","","Completed","2022-12-11T08:00:00","No","No","No","Internal"]
[null,null,null,null,93856,"88_Wed Nov 30 2022 09:53:29 GMT+0800","2022-11-29T08:00:00","Breakdown","Ship Staff","Ship Staff Insp.","Crew lounge WiFi not working.","Accommodation","MLC Related","Equipment Related","11.16","Low","","","The router is not stopped working. IT dept checked and unable to activate it remotely but found that it was an extender and not a router.PO-DEUR220260 Raised. Same received on 14/Nov/2022 and installed. Working satisfactory.","2022-12-11T08:00:00","","Completed","2022-12-15T08:00:00","No","No","No","Internal","Order approved and same will be supplied when vessel calls Singapore."]
[null,null,null,null,95851,"88_Tue Jan 03 2023 17:23:51 GMT+0800","2022-12-16T08:00:00","Observation,Defect","Ship Staff","Ship Staff Insp.","Incinerator: Primary  burner FO pump seal leak","Critical Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Pump replaced. Tried out and working satisfactory.","2022-12-21T08:00:00","","Completed","2022-12-16T08:00:00","No","No","No","Internal"]
[null,null,null,null,59183,"88_Wed Nov 30 2022 09:51:07 GMT+0800","2022-11-29T08:00:00","Breakdown","Ship Staff","Ship Staff Insp.","Boiler suit washing machine not working","Accommodation","MLC Related","Equipment Related","11.16","Low","","","New washing machine received at Khor-fakkan . Already installed & working satisfactory.","2022-12-11T08:00:00","washing machine for crew laundry received under PO no 220263","Completed","2022-12-23T08:00:00","No","No","No","Internal"]
[null,null,null,null,66948,"88_Tue Nov 29 2022 12:29:18 GMT+0800","2022-11-19T08:00:00","Defect","Ship Staff","Ship Staff Insp.","No 2 steering motor and No 3 steering motor does not work at times.","Cargo Mach.","Navigation","Equipment Related","10.39","High","","","On delay contact 6 & 8 malfunctioning. Contact 1 & 3 swiped and now working satisfactory. ","2022-12-31T08:00:00","","Completed","2022-12-24T08:00:00","No","No","No","Internal"]
[null,null,null,null,46444,"88_Wed Aug 31 2022 16:49:41 GMT+0800","2022-08-27T08:00:00","Critical Equipment","Ship Staff","Ship Staff Insp.","Hydraulic hand pump for starting EDG leaking from seal.","Critical Equip.","Emgcy. Systems","Equipment Related","10.32","Very High","","","EMERGENCY GENERATOR HYDRAULIC HAND PUMP to renew.\nHand pump received and replaced. Tried out and found working satisfactory.","2023-01-18T08:00:00","DEUR220196 - EMERGENCY GENERATOR HYDRAULIC HAND PUMP","Completed","2023-01-05T08:00:00","No","No","No","Internal"]
[null,null,null,null,69200,"88_Fri Jan 13 2023 18:59:12 GMT+0800","2023-01-12T08:00:00","Observation","Ship Staff","Ship Staff Insp.","Steering gear: Rudder angle indicator linkage support roller sheared off due to PVC material.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.39","High","","","Support roller fab with aluminium pipe. Function test and rudder angle calibration done. Working satisfactory.","2023-01-18T08:00:00","","Completed","2023-01-13T08:00:00","No","No","No","Internal"]
[null,null,null,null,28102,"88_Sun Jan 15 2023 10:07:31 GMT+0800","2023-01-06T08:00:00","Observation","Ship Staff","Ship Staff Insp.","LT cooler port side: SW inlet line sacrificial flange corroded and leak observed.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Spare sacrificial flange was received earlier. Same replaced and system put back to normal.","2023-01-15T08:00:00","","Completed","2023-01-14T08:00:00","No","No","No","Internal"]
[null,null,null,null,88980,"88_Wed Nov 30 2022 13:02:35 GMT+0800","2022-11-29T08:00:00","Defect","Ship Staff","Ship Staff Insp.","AUS drain tank level gauge is not working","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.45","High","","","Air pressure checked on the regulator side found satisfactory. Operation checked during cargo discharge. Working satisfactory.","2023-01-30T08:00:00","","Completed","2023-01-15T08:00:00","No","No","No","Internal"]
[null,null,null,null,66369,"88_Thu Dec 01 2022 11:28:42 GMT+0800","2022-11-24T08:00:00","Defect","Ship Staff","Ship Staff Insp.","IG topping up generator SW outlet valve connecting to overboard line having soft patch","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","valve received 14/Dec/2022. Job planned in ballast voyage.\nValve renewed. No leaks and put back to normal operations.","2023-01-20T08:00:00","DEUR220265","Completed","2023-01-17T08:00:00","No","No","No","Internal"]
[null,null,null,null,69534,"88_Wed Jan 25 2023 12:00:36 GMT+0800","2023-01-16T08:00:00","Critical Equipment","Ship Staff","Ship Staff Insp.","Incinerator: Primary FO pump leak and not building pressure and sluice door non operational.","Critical Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Primary FO pump & Sluice door solenoid valve replaced. Tried out and working satisfactory.","2023-01-19T08:00:00","","Completed","2023-01-16T08:00:00","No","No","No","Internal"]
[null,null,null,null,65439,"88_Mon Jan 30 2023 16:12:07 GMT+0800","2023-01-24T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Hydraulic oil Leaking from Stbd Side Hose handling Crane Level Gauge Glass.","Deck - Machinery","Cargo / Ballast Systems","Equipment Related","8.50","Medium","","","Level Gauge Glass replace with the New gauge Glass.","2023-02-24T08:00:00","","Completed","2023-01-29T08:00:00","No","No","No","Internal"]
[null,null,null,null,68707,"88_Wed Feb 01 2023 13:15:10 GMT+0800","2023-01-26T08:00:00","Observation","Ship Staff","Ship Staff Insp.","Main air compressor # 2: oil leak from shaft seal.","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Seal replaced. System put back in service. No leaks.","2023-01-30T08:00:00","","Completed","2023-01-28T08:00:00","No","No","No","Internal"]
[null,null,null,null,92227,"88_Wed Feb 01 2023 17:57:38 GMT+0800","2023-01-17T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Hydraulic leak observed on Mooring winch no M7 from Operation lever","Deck - Mooring Machinery","Mooring","Equipment Related","9.14","Medium","","","O rings to be renewed on the Operating lever Block","2023-02-16T08:00:00","","Completed","2023-01-27T08:00:00","No","No","No","Internal"]
[null,null,null,null,71322,"88_Thu Feb 02 2023 12:32:32 GMT+0800","2023-01-28T08:00:00","Critical Equipment","Ship Staff","Ship Staff Insp.","Life boat port: battery charger connector defective. ","Critical Equip.","Safety / LSA / FFA","Equipment Related","5.27","Medium","","","Connector replaced. Working satisfactory","2023-01-28T08:00:00","","Completed","2023-01-28T08:00:00","No","No","No","Internal"]
[null,null,null,null,14069,"88_Mon Feb 06 2023 21:44:37 GMT+0800","2023-01-21T08:00:00","Observation","Ship Staff","Ship Staff Insp.","ME # 2 unit: Stuffing box leak noted about 45.2 ltrs/day.  Scrap down analysis report not normal due to high phosphorus. ","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Stuffing box overhauled in SITU at Khor fakkan anchorage by shore team. Same will be observed during voyage.","2023-02-08T08:00:00","","Completed","2023-02-04T08:00:00","No","No","No","Internal"]
[null,null,null,null,25856,"88_Wed Feb 15 2023 12:59:59 GMT+0800","2023-02-12T08:00:00","Observation","Ship Staff","Ship Staff Insp.","Windlass port: brake cylinder seals leaking.","Deck - Mooring Machinery","Mooring","Equipment Related","9.20","Medium","","","Seals replaced and tried out. No leaks.","2023-02-18T08:00:00","","Completed","2023-02-14T08:00:00","No","No","No","Internal"]
[null,null,null,null,68522,"0_Wed Feb 15 2023 13:04:09 GMT+0800","2023-02-07T08:00:00","Observation","Ship Staff","Ship Staff Insp.","Windlass stbd: brake cylinder seals & Shaft engaging lever seals leaking.","Deck - Mooring Machinery","Mooring","Equipment Related","9.20","Medium","","","Seals & O rings replaced for brake cylinder and shaft engaging lever. Tried out and noted no leaks.","2023-02-07T08:00:00","","Completed","2023-02-07T08:00:00","No","No","No","Internal"]
[null,null,null,null,68506,"88_Tue Jul 19 2022 21:02:40 GMT+0800","2022-11-29T08:00:00","Observation","Ship Staff","Ship Staff Insp.","Starboard bridge wing ME Maneuvering not working due to misalignment with bridge telegraph.  Local telegraph intermittent failure alarm but not effecting the navigation.","Navigation - Others","Navigation","Equipment Related","4.7","High","","","Same replaced by shore team. Simulation test (vessel at anchor) carried out and noted working satisfactory for both bridge wings. \nLocal telegraph: Voltage adjusted to 25V as previously was 24V. Replaced software ic with new one (56002 A5). Two flat cables renewed. \nAt present no alarms in the system.","2023-02-27T08:00:00","DEUR235007","Completed","2023-02-04T08:00:00","No","No","No","Internal"]
[null,null,null,null,20608,"88_Thu Aug 25 2022 16:06:13 GMT+0800","2022-08-21T08:00:00","Observation","Ship Staff","Ship Staff Insp.","Cargo Eductor Discharge pressure not working, showing erratic readings","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.8","Medium","","","Pressure transmitter was overhauled and tested with pressure calibrator but still not showing reading and the reading shown is in error. Spares received 14/Dec/2022. Job completed. Checked during cargo discharge operations. Working satisfactory.","2023-01-31T08:00:00","DEUR220215","Completed","2023-01-12T08:00:00","No","No","No","Internal"]
[null,null,null,null,28301,"88_Fri Nov 11 2022 08:29:52 GMT+0800","2022-11-02T08:00:00","Defect","Ship Staff","Ship Staff Insp.","When DGPS nO 1 OR no 2 is Selected for position output, the gyro output disappears from all equipment and alarms are generated E03.4 on Autopilot and \"d\" on Gyro panel. Then the other DGPS output must be selected to silence alarms.","Navigation - DGPS / EPFS / AIS","Navigation","Equipment Related","4.17","Very High","","","Checking the circuits., as advised from office.\nThe voltage from #3 DGPS output buffer to gyro compass at terminals 10A 10B was measured during alarm condition and found 3.2vdc fluctuating,\nand there was no alarm on any other equipment connected to #3 DGPS o/p buffer.\nAfter changing over  to #1 DGPS the alarm was activated again. The alarm was reset and changed over to #2 DGPS and there was no alarm.\nDGPS #2 is still in use and working without any alarm.\nAll connections retightened. No alarms since last 15 days.","2023-02-04T08:00:00","","Completed","2023-02-01T08:00:00","No","No","No","Internal"]
[null,null,null,null,53475,"88_Wed Feb 15 2023 14:46:59 GMT+0800","2023-02-15T08:00:00","Breakdown","Ship Staff","Ship Staff Insp.","Aux SW pump: mech seal leakage","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Mech seal replaced and tried out. Satisfactory.","2023-02-15T08:00:00","","Completed","2023-02-15T08:00:00","No","No","No","Internal"]
[null,null,null,22674,null,"88_19-11-2021 09:39:20","2021-11-10T08:00:00","Defect","Ship Staff","Ship Staff Insp.","BWTS No.2 Filter - 1pc Filter Element damaged/holed (Total element per set = 54pcs).","Miscellaneous","Cargo / Ballast Systems","Equipment Related","6.22","Medium","","","RO DEUR220003 raised. Replaced holed / damaged filter element with newly received.","2023-02-28T08:00:00","DEUR220003","Completed","2023-02-21T08:00:00","No","No","No","Internal","Will be arranged at convenient port."]
[null,null,null,null,82506,"88_Sun Feb 26 2023 09:20:33 GMT+0800","2023-02-23T08:00:00","Defect","Ship Staff","Ship Staff Insp.","COPT # 2 AUS pneumatic discharge valve not operating remotely from CCR","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.8","Medium","","","On inspection found indicator linkage wheel shaft had sheared off from end part. Only manual operation was possible from pump room. New piece welded in place. Gear wheel also damaged in one section. Fixed back and adjusted the opening and closing settings. Remote operation from CCR tried out and working satisfactory. Requisition raised for one spare pneumatic controller,","2023-02-27T08:00:00","","Completed","2023-02-25T08:00:00","No","No","No","Internal"]
[null,null,null,null,23084,"88_Tue Nov 15 2022 20:43:59 GMT+0800","2022-10-31T08:00:00","Defect","Ship Staff","Ship Staff Insp.","VRCS pumps discharge line relief valve found leaking.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.11","Medium","","","relief valve opened and inspected. Found slightly leaking. Req # DEUR220256 raised. Valve received and replaced.","2023-02-28T08:00:00","DEUR220256","Completed","2023-02-21T08:00:00","No","No","No","Internal"]
[null,null,null,null,46550,"88_Thu Aug 25 2022 16:09:33 GMT+0800","2022-08-21T08:00:00","Observation","Ship Staff","Ship Staff Insp.","Hydro-blaster not working due to pressure switch faulty","Miscellaneous","General Appearance","Equipment Related","11.1","High","","","Pressure switch replaced. Pump impeller inspected and noted 3 to 4 blades twisted. As advised, replaced with new version valves and tried out. The centrifugal pump is building pressure upto 2.0 bar, but as per makers it should be 4.0 bar.  Contactor ratings fitted is of lesser capacity (39A).  As per manual it should be 52A. The motor starts on star connection and the pressure build up is around 500 bar and stops before changing over to delta. Awaiting response from office/maker if new rated contactor / overload relay (52A)  can be fitted and system tried out.\nFound one phase of delta connection isolated, and both ends of one phase connected to same line. \nPreviously the connection was : [u1- w2 , v1-v2, w1- u2]\nCorrected connection : [ u1-w2, v1-u2, w1-v2]\nNo contactors and Overcurrent relays replaced.\nTried out the Hydro blaster, motor changed over to delta and drawing phase current 21A.\nBuild-up of pressure is approx. 560 bar and working satisfactory.\nCentrifugal pump pressure 2.4 bar, but should be 4.0 bar as per maker’s.\nVessel will try out in the ballast passage after the block leaks are rectified and nozzle replaced.","2023-02-28T08:00:00","","Completed","2023-02-25T08:00:00","No","No","No","Internal"]
[null,null,null,null,17064,"88_Tue Mar 14 2023 13:38:22 GMT+0800","2023-03-09T08:00:00","Defect","Ship Staff","Ship Staff Insp.","AC Comp no 2 discharge guage defective and leaking ,need to be replaced.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","Pressure guage renewed with the spare received.","2023-03-15T08:00:00","","Completed","2023-03-11T08:00:00","No","No","No","Internal"]
[null,null,null,null,13963,"0_Tue Mar 14 2023 13:42:18 GMT+0800","2023-03-07T08:00:00","Critical Equipment","Ship Staff","Ship Staff Insp.","Emergency DG Co2 Cabinet door hinges wasted/ Weathered out.","Critical Equip.","Emgcy. Systems","Equipment Related","5.40","Very High","","","Door brought back to engine room workshop new hinges fabricated.","2023-03-14T08:00:00","","Completed","2023-03-10T08:00:00","No","No","No","Internal"]
[null,null,null,null,39536,"0_Tue Mar 14 2023 13:49:42 GMT+0800","2023-03-04T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Copt no 2 lube oil line leaky","E/R - Pipes/ valves & fittings","Cargo / Ballast Systems","Equipment Related","8.8","Medium","","","Pipe replaced with spare one.","2023-03-14T08:00:00","","Completed","2023-03-13T08:00:00","No","No","No","Internal"]
[null,null,null,null,80856,"0_Tue Mar 14 2023 13:55:19 GMT+0800","2023-03-07T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Smoke detectors for boiler No.1 Zone 2 sensor 12 and  and ME Zone 1 smoke sensor 2 of Hyper mist system found faulty.","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.35","Medium","","","Troubleshooting and subsequent replacement of smoke detectors for boiler No.1 Zone 2 sensor 12 and  and ME Zone 1 smoke sensor 2 of Hyper mist system\nworking satisfactory","2023-03-09T08:00:00","","Completed","2023-03-08T08:00:00","No","No","No","Internal"]
[null,null,null,null,28736,"0_Tue Mar 14 2023 14:00:19 GMT+0800","2023-03-03T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Aux Boiler No 1 water controller for 20 k malfunction.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Service engineer replaced diaphgram with a new one. ","2023-03-10T08:00:00","","Completed","2023-03-07T08:00:00","No","No","No","Internal"]

{"sheet":"Calc","index":2,"n_rows":28,"n_cols":12,"rows_kept":28,"cut":false,"hidden":true,"merged":[]}
["Def_type","Def_cause","Equipments","VIQrefno","Observer_code"]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,"Dim itemSele As Long"]
[null,null,null,null,null,null,null,null,null,null,null,"   dim startRow as integer"]
[null,null,null,null,null,null,null,null,null,null,null,"   startRow=1"]
[null,null,null,null,null,null,null,null,null,null,null,"        For itemSele = 0 To ListBox1.ListCount - 1"]
[null,null,null,null,null,null,null,null,null,null,null,"        If ListBox1.Selected(itemSele) = True Then"]
[null,null,null,null,null,null,null,null,null,null,null,"        Worksheets(\"WorksheetName\").Range(\"A\" & startRow).Value = ListBox1.List(itemSele)"]
[null,null,null,null,null,null,null,null,null,null,null,"        startRow = startRow + 1"]
[null,null,null,null,null,null,null,null,null,null,null,"        End If"]
[null,null,null,null,null,null,null,null,null,null,null,"        Next"]
[null,null,null,null,null,null,null,null,null,null,null,"Dim LastRowA As String"]
[null,null,null,null,null,null,null,null,null,null,null,"        Dim itemSele As Long"]
[null,null,null,null,null,null,null,null,null,null,null,"       Dim startRow as integer"]
[null,null,null,null,null,null,null,null,null,null,null,"        LastRowA = ActiveSheet.Cells(Rows.count, \"A\").End(xlUp).row"]
[null,null,null,null,null,null,null,null,null,null,null,"        startQue = 0"]
[null,null,null,null,null,null,null,null,null,null,null,"        For itemSele = 0 To ListBox1.ListCount - 1"]
[null,null,null,null,null,null,null,null,null,null,null,"        For startRow = 1 To LastRowA"]
[null,null,null,null,null,null,null,null,null,null,null,"        If Worksheets(\"WorksheetName\").Range(\"A\" & startRow).Value = ListBox1.List(itemSele) Then"]
[null,null,null,null,null,null,null,null,null,null,null,"        ListBox1.Selected(itemSele) = True"]
[null,null,null,null,null,null,null,null,null,null,null,"        Exit For"]
[null,null,null,null,null,null,null,null,null,null,null,"        End If"]
[null,null,null,null,null,null,null,null,null,null,null,"        Next j"]
[null,null,null,null,null,null,null,null,null,null,null,"        Next"]
[null,null,null,null,null,null,null,null,null,null,null,"        End If"]

{"sheet":"Areaofobs","index":3,"n_rows":17,"n_cols":2,"rows_kept":17,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Cargo / Ballast Systems",11]
["Cert. & Docu.",2]
["Communication",6]
["Crew Management",3]
["Emgcy. Systems",13]
["Eng. / Strg. Comp.",14]
["General Appearance",15]
["Ice Opns.",17]
["ISM Related",7]
["ISPS Related",10]
["MARPOL Related",9]
["MLC Related",4]
["Mooring",12]
["Navigation",5]
["Safety / LSA / FFA",8]
["Structural Condn. / WT integrity ",16]

{"sheet":"Vessel_type","index":4,"n_rows":1,"n_cols":2,"rows_kept":1,"cut":false,"hidden":true,"merged":[]}
["Vessel_type","ID"]

{"sheet":"Deficiency_type","index":5,"n_rows":8,"n_cols":3,"rows_kept":8,"cut":false,"hidden":true,"merged":[]}
["TITLE","Type of deficiency_description","ID"]
["Breakdown",null,6]
["Critical Equipment",null,4]
["Defect",null,1]
["Guarantee Claim",null,8]
["Non Conformity",null,2]
["Observation",null,3]
["Other",null,7]

{"sheet":"VIQrefno","index":6,"n_rows":427,"n_cols":3,"rows_kept":427,"cut":false,"hidden":true,"merged":[]}
["VIQ_ref_no","Risk Value of observation","ID"]
["1.1","Low",8243]
["1.10","Low",8252]
["1.11","Low",8253]
["1.12","Low",8254]
["1.13","Low",8255]
["1.14","Low",8256]
["1.15","Low",8257]
["1.16","Low",8259]
["1.17","Low",8260]
["1.18","Low",8261]
["1.19","Low",8262]
["1.2","Low",8244]
["1.20","Low",8263]
["1.21","Low",8265]
["1.22","Low",8266]
["1.23","Low",8267]
["1.24","Low",8268]
["1.25","Low",8269]
["1.26","Low",8270]
["1.3","Low",8245]
["1.4","Low",8246]
["1.5","Low",8247]
["1.6","Low",8248]
["1.7","Low",8249]
["1.8","Low",8250]
["1.9","Low",8251]
["1.99","High",11258]
["10.1","Medium",8461]
["10.10","High",8470]
["10.11","Medium",8471]
["10.12","Very High",8472]
["10.13","Very High",8473]
["10.14","Medium",8474]
["10.15","Low",8475]
["10.16","Very High",8476]
["10.17","Very High",8477]
["10.18","High",8478]
["10.19","Very High",8479]
["10.2","Low",8462]
["10.20","High",8480]
["10.21","Medium",8481]
["10.22","Low",8482]
["10.23","Medium",8483]
["10.24","Low",8484]
["10.25","Very High",8485]
["10.26","High",8486]
["10.27","Medium",8487]
["10.28","Low",8488]
["10.29","Medium",8489]
["10.3","Medium",8463]
["10.30","High",8490]
["10.31","Very High",8491]
["10.32","Very High",8492]
["10.33","High",8493]
["10.34","High",8494]
["10.35","Very High",8495]
["10.36","Very High",8496]
["10.37","Medium",8497]
["10.38","Medium",8498]
["10.39","High",8499]
["10.4","High",8464]
["10.40","Medium",8500]
["10.41","Medium",8501]
["10.42","Medium",8502]
["10.43","Medium",8503]
["10.44","Medium",8504]
["10.45","Very High",8505]
["10.46","High",8506]
["10.47","Medium",8507]
["10.48","High",8508]
["10.49","Medium",8509]
["10.5","Low",8465]
["10.50","High",8510]
["10.51","Low",8511]
["10.52","Medium",8512]
["10.53","Medium",8513]
["10.54","High",8514]
["10.55","Low",8515]
["10.6","Very High",8466]
["10.7","Medium",8467]
["10.8","Medium",8468]
["10.9","Medium",8469]
["10.99","High",8516]
["11.1","High",8420]
["11.10","Medium",8429]
["11.11","Very High",8430]
["11.12","Low",8431]
["11.13","Low",8432]
["11.14","Medium",8433]
["11.15","Low",8434]
["11.16","Low",8435]
["11.17","Low",8436]
["11.2","Medium",8421]
["11.3","Medium",8422]
["11.4","Very High",8423]
["11.5","Medium",8424]
["11.6","Medium",8425]
["11.7","High",8426]
["11.8","Low",8427]
["11.9","Low",8428]
["11.99","High",8437]
["12.1","High",8438]
["12.10","High",8448]
["12.11","High",8449]
["12.12","High",8450]
["12.13","High",8451]
["12.14","High",8452]
["12.15","High",8453]
["12.16","High",8454]
["12.17","High",8455]
["12.18","High",8456]
["12.19","High",8457]
["12.2","High",8439]
["12.20","High",8458]
["12.21","High",8459]
["12.3","High",8441]
["12.4","High",8442]
["12.5","High",8443]
["12.6","High",8444]
["12.7","High",8445]
["12.8","High",8446]
["12.9","High",8447]
["12.99","High",8460]
["2.1","Very High",8296]
["2.1.9","Very High",11259]
["2.10","Medium",8304]
["2.11","Medium",8305]
["2.12","Low",8306]
["2.13","Low",8307]
["2.14","Low",8308]
["2.15","Low",8309]
["2.16","Medium",8310]
["2.2","Medium",8297]
["2.3","High",8295]
["2.4","Medium",8298]
["2.5","Medium",8299]
["2.6","Low",8300]
["2.7","High",8301]
["2.8","High",8302]
["2.9","Medium",8303]
["2.99","High",8311]
["3.1","High",8312]
["3.2","Very High",8313]
["3.3","High",8314]
["3.4","Low",8294]
["3.5","Medium",8315]
["3.6","High",8316]
["3.7","Very High",8317]
["3.8","Very High",8318]
["3.99","High",8319]
["4.1","High",8320]
["4.10","High",8329]
["4.11","Medium",8330]
["4.12","Very High",8331]
["4.13","Very High",8332]
["4.14","Very High",8333]
["4.15","Very High",8334]
["4.16","Very High",8335]
["4.17","Very High",8336]
["4.18","Very High",8337]
["4.19","Low",8338]
["4.2","Medium",8321]
["4.20","Very High",8339]
["4.21","High",8340]
["4.22","Low",8341]
["4.23","High",8342]
["4.24","High",8343]
["4.25","Low",8344]
["4.26","Low",8345]
["4.27","High",8346]
["4.3","Medium",8322]
["4.4","High",8323]
["4.5","Very High",8324]
["4.6","Medium",8325]
["4.7","High",8326]
["4.8","Medium",8327]
["4.9","Medium",8328]
["4.99","High",8347]
["5.1","Very High",8517]
["5.10","High",8526]
["5.11","Low",8527]
["5.12","Medium",8528]
["5.13","High",8529]
["5.14","Very High",8530]
["5.15","Medium",8531]
["5.16","Very High",8532]
["5.17","Very High",8533]
["5.18","High",8534]
["5.19","Medium",8535]
["5.2","Very High",8518]
["5.20","Medium",8536]
["5.21","Medium",8537]
["5.22","High",8539]
["5.23","Very High",8540]
["5.24","Very High",8541]
["5.25","Medium",8542]
["5.26","Medium",8543]
["5.27","Medium",8544]
["5.28","Very High",8545]
["5.29","High",8546]
["5.3","Low",8519]
["5.30","High",8547]
["5.31","High",8548]
["5.32","High",8549]
["5.33","High",8550]
["5.34","Low",8551]
["5.35","Medium",8552]
["5.36","Low",8553]
["5.37","Low",8554]
["5.38","High",8555]
["5.39","Very High",8556]
["5.4","High",8520]
["5.40","Very High",8557]
["5.41","Very High",8558]
["5.42","Medium",8559]
["5.43","High",8560]
["5.44","High",8561]
["5.45","Medium",8564]
["5.46","Medium",8565]
["5.47","Medium",8566]
["5.48","Medium",8567]
["5.5","Low",8521]
["5.6","Low",8522]
["5.7","Medium",8523]
["5.8","Medium",8524]
["5.9","Very High",8525]
["5.99","High",8568]
["6.1","Medium",8348]
["6.10","Low",8357]
["6.11","High",8358]
["6.12","Medium",8359]
["6.13","Low",8360]
["6.14","High",8361]
["6.15","High",8362]
["6.16","Very High",8363]
["6.17","Very High",8364]
["6.18","Medium",8365]
["6.19","Low",8366]
["6.2","High",8349]
["6.20","Medium",8367]
["6.21","High",8368]
["6.22","Medium",8369]
["6.3","Low",8350]
["6.4","High",8351]
["6.5","Medium",8352]
["6.6","Medium",8353]
["6.7","High",8354]
["6.8","High",8355]
["6.9","Low",8356]
["6.99","High",8370]
["7.1","High",8371]
["7.10","High",8380]
["7.11","High",8381]
["7.12","High",8382]
["7.13","Medium",8383]
["7.14","Medium",8384]
["7.15","High",8385]
["7.16","High",8386]
["7.17","High",8387]
["7.2","High",8372]
["7.3","Low",8373]
["7.4","Low",8374]
["7.5","Low",8375]
["7.6","Medium",8376]
["7.7","Low",8377]
["7.8","High",8378]
["7.9","High",8379]
["7.99","High",8388]
["8.1","Very High",8569]
["8.10","Very High",8578]
["8.100","Low",11227]
["8.101","Medium",11228]
["8.102","Low",11229]
["8.103","Low",11230]
["8.104","Low",11231]
["8.105","Medium",11232]
["8.106","Medium",11233]
["8.107","Low",11234]
["8.108","High",11235]
["8.109","Very High",11236]
["8.11","Medium",8579]
["8.110","High",11237]
["8.111","Medium",11238]
["8.112","High",11239]
["8.113","Medium",11240]
["8.114","Low",11241]
["8.115","High",11242]
["8.116","Medium",11243]
["8.117","Medium",11244]
["8.118","Medium",11245]
["8.119","High",11246]
["8.12","Medium",8580]
["8.120","High",11247]
["8.121","Medium",11248]
["8.122","High",11249]
["8.123","High",11250]
["8.124","Low",11251]
["8.125","High",11252]
["8.126","Medium",11253]
["8.127","Medium",11254]
["8.13","Medium",8581]
["8.14","Very High",8582]
["8.15","High",8583]
["8.16","Very High",8584]
["8.17","Low",8585]
["8.18","High",8586]
["8.19","High",8587]
["8.199","High",11255]
["8.2","Medium",8570]
["8.20","Medium",8588]
["8.21","High",8589]
["8.22","Very High",8590]
["8.23","Medium",8591]
["8.24","Medium",8592]
["8.25","Very High",8593]
["8.26","High",8594]
["8.27","Medium",8595]
["8.28","Medium",8596]
["8.29","High",8598]
["8.3","Very High",8571]
["8.30","High",8599]
["8.31","High",8600]
["8.32","Low",8601]
["8.33","Medium",8602]
["8.34","High",8603]
["8.35","Medium",8604]
["8.36","Medium",8605]
["8.37","High",8607]
["8.38","Medium",8608]
["8.39","Medium",8609]
["8.4","Medium",8572]
["8.40","High",8610]
["8.41","Medium",8611]
["8.42","Medium",8612]
["8.43","Very High",8613]
["8.44","High",8615]
["8.45","High",8616]
["8.46","Very High",8617]
["8.47","Very High",8618]
["8.48","Medium",8619]
["8.49","High",8620]
["8.5","Very High",8573]
["8.50","Medium",8621]
["8.51","Low",8622]
["8.52","Low",8623]
["8.53","Low",8624]
["8.54","High",8625]
["8.55","Low",11182]
["8.56","Medium",11183]
["8.57","Medium",11184]
["8.58","High",11185]
["8.59","High",11186]
["8.6","Medium",8574]
["8.60","High",11187]
["8.61","Medium",11188]
["8.62","Very High",11189]
["8.63","High",11190]
["8.64","Medium",11191]
["8.65","Low",11192]
["8.66","High",11193]
["8.67","High",11194]
["8.68","High",11195]
["8.69","Medium",11196]
["8.7","High",8575]
["8.70","Medium",11197]
["8.71","Very High",11198]
["8.72","Medium",11199]
["8.73","Medium",11200]
["8.74","High",11201]
["8.75","Medium",11202]
["8.76","Medium",11203]
["8.77","Medium",11204]
["8.78","Medium",11205]
["8.79","Medium",11206]
["8.8","Medium",8576]
["8.80","Medium",11207]
["8.81","Low",11208]
["8.82","Medium",11209]
["8.83","Low",11210]
["8.84","Low",11211]
["8.85","Medium",11212]
["8.86","Medium",11213]
["8.87","Medium",11214]
["8.88","Low",11215]
["8.89","High",11216]
["8.9","High",8577]
["8.90","High",11217]
["8.91","High",11218]
["8.92","Medium",11219]
["8.93","Low",11220]
["8.94","Low",11221]
["8.95","Medium",11222]
["8.96","Medium",11223]
["8.97","Low",11224]
["8.98","High",11225]
["8.99","Medium",11226]
["9.1","Low",8390]
["9.10","Medium",8399]
["9.11","Medium",8400]
["9.12","Medium",8401]
["9.13","Low",8402]
["9.14","Medium",8403]
["9.15","Medium",8404]
["9.16","High",8405]
["9.17","High",8406]
["9.18","Low",8407]
["9.19","Low",8408]
["9.2","Very High",8391]
["9.20","Medium",8409]
["9.21","Medium",8410]
["9.22","Low",8411]
["9.23","Low",8412]
["9.24","Medium",8413]
["9.25","Low",8414]
["9.26","Low",8415]
["9.27","Low",8416]
["9.28","Medium",8417]
["9.29","Low",8418]
["9.3","Very High",8392]
["9.4","High",8393]
["9.5","High",8394]
["9.6","Low",8395]
["9.7","Medium",8396]
["9.8","Medium",8397]
["9.9","Medium",8398]
["9.99","High",8419]

{"sheet":"Equipment_list","index":7,"n_rows":28,"n_cols":3,"rows_kept":28,"cut":false,"hidden":true,"merged":[]}
["TITLE","Equipment_list_description","ID"]
["Accommodation",null,12]
["Cargo Mach.",null,13]
["Critical Equip.",null,16]
["Deck - Machinery",null,18]
["Deck - Mooring Machinery",null,15]
["Deck - Pipe / Fittings",null,20]
["Documentation",null,21]
["E/R - Air Comp.",null,8]
["E/R - Aux. Engine",null,4]
["E/R - Aux. Mach.",null,7]
["E/R - Boiler",null,5]
["E/R - Main Engine",null,3]
["E/R - Pipes/ valves & fittings",null,9]
["E/R - Pumps",null,32]
["E/R - Purifier",null,6]
["Elect. Mach. & Equip.",null,10]
["Hull & Tanks",null,19]
["Inert Gas",null,14]
["LSA / FFA",null,17]
["Miscellaneous",null,22]
["Navigation - DGPS / EPFS / AIS",null,28]
["Navigation - ECDIS",null,25]
["Navigation - Echo Sounder / Speed Log",null,26]
["Navigation - GMDSS & Communication",null,23]
["Navigation - Others",null,11]
["Navigation - RADAR",null,24]
["Navigation - VDR / BNWAS",null,30]

{"sheet":"PSC_MOU","index":8,"n_rows":11,"n_cols":3,"rows_kept":11,"cut":false,"hidden":true,"merged":[]}
["TITLE","PSC_MOU_description","ID"]
["Asia and the Pacific",null,2]
["Caribbean",null,4]
["Europe and the North Atlantic",null,1]
["Latin America",null,3]
["The Black Sea region",null,6]
["The Indian Ocean",null,8]
["The Mediterranean",null,7]
["The Riyadh MoU",null,9]
["USCG",null,10]
["West and Central Africa",null,5]

{"sheet":"Inspection_type","index":9,"n_rows":13,"n_cols":2,"rows_kept":13,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Bunkering Audit",14]
["Cargo Audit",17]
["Engineering Audit",16]
["ISM Audit",2]
["ISPS Audit",3]
["IT Audit",10]
["MLC Audit",1]
["Mooring Audit",9]
["Nav Audit / Verification",8]
["Onboard Training",18]
["Ship Staff Insp.",15]
["Suptd. Insp.",13]

{"sheet":"Deficiency_Cause","index":10,"n_rows":8,"n_cols":3,"rows_kept":8,"cut":false,"hidden":true,"merged":[]}
["TITLE","Deficiency_Cause_description","ID"]
["Behaviour Based",null,1]
["Equipment Related",null,4]
["External Factors",null,5]
["Human Error",null,7]
["Inappropriate Procedure",null,8]
["Industry Issue",null,6]
["Knowledge Based",null,3]

{"sheet":"Observer_code","index":11,"n_rows":3,"n_cols":3,"rows_kept":3,"cut":false,"hidden":true,"merged":[]}
["TITLE","Observer_code_description","ID"]
["Owner / Marine / Tech. Suptd.",null,3]
["Ship Staff",null,2]

{"sheet":"Status_code","index":12,"n_rows":6,"n_cols":3,"rows_kept":6,"cut":false,"hidden":true,"merged":[]}
["TITLE","Status_code_description","ID"]
["Completed",null,6]
["Deferred to D D",null,5]
["In progress",null,3]
["Not Started",null,2]
["Waiting spare",null,4]

{"sheet":"PSC_ref_no","index":13,"n_rows":19,"n_cols":2,"rows_kept":19,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Alarms",9]
["Cargo operations including equipment",7]
["Certificates & Documentation",2]
["Dangerous Goods",13]
["Emergency Systems",5]
["Fire safety",8]
["ISM",16]
["ISPS",17]
["Life saving appliances",12]
["MLC, 2006",18]
["Other",19]
["Pollution Prevention",15]
["Propulsion and auxiliary machinery",14]
["Radio communication",6]
["Safety of Navigation",11]
["Structural condition",3]
["Water/Weathertight condition",4]
["Working and Living Conditions",10]

{"sheet":"Risk_value_of_obs","index":14,"n_rows":1,"n_cols":2,"rows_kept":1,"cut":false,"hidden":true,"merged":[]}
["Risk Value of observation","ID"]

{"sheet":"Year","index":15,"n_rows":18,"n_cols":1,"rows_kept":18,"cut":false,"hidden":true,"merged":[]}
["Year"]
[2014]
[2015]
[2016]
[2017]
[2018]
[2019]
[2020]
[2021]
[2022]
[2023]
[2024]
[2025]
[2026]
[2027]
[2028]
[2029]
[2030]

{"sheet":"Month","index":16,"n_rows":13,"n_cols":1,"rows_kept":13,"cut":false,"hidden":true,"merged":[]}
["Month"]
["Jan"]
["Feb"]
["Mar"]
["Apr"]
["May"]
["Jun"]
["Jul"]
["Aug"]
["Sep"]
["Oct"]
["Nov"]
["Dec"]

{"sheet":"Date_","index":17,"n_rows":32,"n_cols":1,"rows_kept":32,"cut":false,"hidden":true,"merged":[]}
["Date"]
["01"]
["02"]
["03"]
["04"]
["05"]
["06"]
["07"]
["08"]
["09"]
[10]
[11]
[12]
[13]
[14]
[15]
[16]
[17]
[18]
[19]
[20]
[21]
[22]
[23]
[24]
[25]
[26]
[27]
[28]
[29]
[30]
[31]

{"sheet":"Sheet1","index":18,"n_rows":24,"n_cols":6,"rows_kept":24,"cut":false,"hidden":true,"merged":[]}
[]
[null,"ID","E",null,"Date Recorded",1]
[null,"UNIQUE ID","F",null,"Type of Deficiency",2]
[1,"Date Recorded","G",null,"Observer code",3]
["ignore","Vessel Type","H",null,"Type of Inspection",4]
[null,"Internal / External","I",null,"Description of Deficiency",5]
[null,"Drydock","J",null,"Equipment Categories",6]
[null,"Information Sharing","K",null,"Area of Observation",7]
[null,"Critical_item","L",null,"Deficiency Cause",8]
[null,"Deficiency Type","M",null,"VIQ Ref Number",9]
[null,"Deficiency Cause","N",null,"Risk Value of Obs",10]
[null,"Inspection Type","O",null,"PSC Ref Number",11]
[null,"Equipments","P",null,"PSC MOU ID",12]
[null,"VIQ Reference Number","Q",null,"Action Taken or Required",13]
[null,"Risk Value of the observation","R",null,"Target Date",14]
[null,"PSC Reference Number","S",null,"PO Ref No.",15]
[null,"PSC MOU","T",null,"Status Code",16]
[null,"Observer Code","U",null,"Date Completed",17]
[null,"Target Date","V",null,"Drydock",18]
[null,"Status Code","W",null,"Info Sharing",19]
[null,"Description of Deficiency","X",null,"Critical Item Flag",20]
[null,"Action taken / required","Y",null,"Audit Type",21]
[null,"PO ref no","Z"]
[null,"Date completed","AA"]

{"sheet":"Ship_information","index":19,"n_rows":2,"n_cols":3,"rows_kept":2,"cut":false,"hidden":true,"merged":[]}
["Ship_ID","Ship_Name","FILE_NAME"]
["88","DHT EUROPE (02-12-2022)","88_1670377765025.xlsm"]

{"sheet":"External_Deficiency_type","index":20,"n_rows":5,"n_cols":3,"rows_kept":5,"cut":false,"hidden":true,"merged":[]}
["TITLE","Type of deficiency_description","ID"]
["Condn of Class / Memo",null,5]
["Defect",null,1]
["Non Conformity",null,2]
["Observation",null,3]

{"sheet":"External_Inspection_type","index":21,"n_rows":11,"n_cols":2,"rows_kept":11,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Cargo Audit",17]
["Flag State Insp.",5]
["ISM Audit",2]
["ISPS Audit",3]
["MLC Audit",1]
["Nav Audit / Verification",8]
["OM Insp. (Eg. SIRE / CDI etc.)",6]
["Others (Eg. Insurance etc.)",12]
["PSC Inspection",4]
["Terminal Insp.",11]

{"sheet":"External_Observer_code","index":22,"n_rows":7,"n_cols":3,"rows_kept":7,"cut":false,"hidden":true,"merged":[]}
["TITLE","Observer_code_description","ID"]
["Class Surveyor",null,4]
["FSC Inspector",null,5]
["Others (Eg. Insurance etc.)",null,9]
["PSC Insp.",null,6]
["SIRE / CDI Insp.",null,8]
["Terminal Insp.",null,7]

{"sheet":"Sheet Version","index":23,"n_rows":2,"n_cols":2,"rows_kept":2,"cut":false,"hidden":true,"merged":[]}
["Version","Title"]
["2.0","Version 2.0"]