{"text_format":"1","workbook":"xlsx","n_sheets":24,"sheets":["Mainsheet","Completed","Calc","Areaofobs","Vessel_type","Deficiency_type","VIQrefno","Equipment_list","PSC_MOU","Inspection_type","Deficiency_Cause","Observer_code","Status_code","PSC_ref_no","Risk_value_of_obs","Year","Month","Date_","Sheet1","Ship_information","External_Deficiency_type","External_Inspection_type","External_Observer_code","Sheet Version"],"not_rendered":{"charts":0,"images":1,"macros":1,"external_links":0,"defined_names":12,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Mainsheet","index":0,"n_rows":26,"n_cols":28,"rows_kept":26,"cut":false,"hidden":false,"merged":[[10,8,10,9],[10,12,10,13],[12,6,12,27],[8,6,8,27]]}
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,"Defect - Damage Monitoring Sheet"]
[]
[null,null,null,null,null,null,null,"Date of Report","01-Jun-2023",null,null,"Ship Name","DHT STALLION (31-05-2023)"]
[]
[null,null,null,null,null,null,"VERSION : 2.0"]
[]
[]
[]
[null,null,null,"ID","SHIPSIDE UNIQUEID","UNIQUE ID","Date Recorded","Type of Deficiency","Observer code","Type of Inspection","Description of Deficiency","Equipment Categories","Area of Observation","Deficiency Cause","VIQ Ref Number","Risk Value of Obs","PSC Ref Number","PSC MOU ID","Action Taken or Required","Target Date","PO Ref No.","Status Code","Date Completed","Drydock","Info Sharing","Critical Item","Audit Type","Superintendent Remarks"]
[null,null,null,28211,36672,"57_Wed Dec 28 2022 23:10:51 GMT+0800","2022-11-24T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","BWTS cell leaking, mainly while washing","E/R - Aux. Mach.","Cargo / Ballast Systems","Equipment Related","10.32","Very High","","","maker advise to be obtained for proper corrective action","2023-07-29T23:59:35","","In progress",null,"No","No","No","Internal","Noted, monitor closely. Try to maintain pressure as low as possible."]
[null,null,null,23335,null,"57_20/12/2021 3:10:18 PM","2022-12-16T23:59:35","Defect","Ship Staff","Ship Staff Insp.","ECR PACKAGED AC UNIT BLDC DRIVER PCB AND FAN UNIT DEFECTIVE.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related,External Factors,Inappropriate Procedure","10.32","Very High","",""," PCB AND FAN UNIT  received DSTA230006 TO BE RENEWED.","2023-06-26T23:59:35","DSTA230006","In progress",null,"No","No","No","Internal","Maker will be supplying spare under warranty."]
[null,null,null,25773,null,"57_18/6/2022 7:31:51 PM","2022-12-25T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Minor quantity of LO traces in LT expansion tank. Suspect ME LO cooler gasket is leaking","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","ME LO cooler plates pressure testing carried out on both LO & FW side, no signs of leak noted.","2023-08-29T23:59:35","","In progress",null,"No","No","No","Internal","LO cooler will be overhauled at DD."]
[null,null,null,25771,null,"57_18/6/2022 7:22:55 PM","2022-12-26T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Vessel call sign to be changed to new Call Sign VRSX9 in BWTS Software system by the makers","Miscellaneous","Cargo / Ballast Systems","Equipment Related","8.18","High","","","Awaiting maker to access BWTS monitor by remote access and change the Call Sign","2023-07-29T23:59:35","","Not Started",null,"No","No","No","Internal"]
[null,null,null,28989,43414,"57_Wed Feb 15 2023 17:22:46 GMT+0800","2023-02-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Port provision crane slewing limit valve block leaking.","Deck - Machinery","Cargo / Ballast Systems","Equipment Related","10.36","Very High","","","New limit switched received under DSTA230010, however noted the installation is different. Need to order limit valve block as a complete unit for renewal.  Communication with supplier in progress.","2023-06-28T23:59:35","DSTA230010","Waiting spare",null,"No","No","No","Internal","Checking with vendor."]
[null,null,null,28990,18703,"57_Wed Feb 15 2023 17:25:06 GMT+0800","2023-02-02T23:59:35","Defect","Ship Staff","Ship Staff Insp.","DG #2 LO centrifuge filter observed not operation.","E/R - Aux. Engine,E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.36","Very High","","","Centrifuge filter was replaced by spare from different maker in the past, still no rotation of the centrifuge observed. DSTA230105 HAS BEEN RAISED FOR NEW lo CENTRIFUGE FILTER","2023-06-28T23:59:35","DSTA230105","Waiting spare",null,"No","No","No","Internal","Raise RO for new LO centrifuge filter."]
[null,null,null,28988,25053,"57_Wed Feb 15 2023 17:18:46 GMT+0800","2023-02-08T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Both Aux boilers Feed control valves operation erratic.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.36","Very High","","","Aux boiler #1 actuator mechanism damaged, same has been order under DSTA230032 was raised in Jan 2023 for spare actuator.\nAux boiler #2 feed water controller actuator working fine in AUTO mode, however noted motor getting hot.","2023-06-28T23:59:35","DSTA230032","Waiting spare",null,"No","No","No","Internal","Noted, will process this requisition."]
[null,null,null,29890,24700,"57_Wed Mar 15 2023 09:31:57 GMT+0800","2023-03-12T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Stbd FW tank level gauge malfunction.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.36","Very High","","","Gauge connecting line checked, and fitted back.  Now showing value with varying offset. Need to raise RO for spare level gauge. \nDSTA230104 has been raised for spare level gauge","2023-06-28T23:59:35","\nDSTA230104","Waiting spare",null,"No","No","No","Internal","Raise RO for required spares."]
[null,null,null,null,65116,"57_Mon May 15 2023 22:44:07 GMT+0800","2023-05-13T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Cargo tank 1P overfill alarm noted not triggering","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","1.5","Low","","","Overfill alarm inspected, found reed switch malfunctioning. Reed switches from other spare floats checked and installed for COT 1P. Overfill alarm tried out confirm alarm operational. DSTA230108 has been raised for spare reed switches.","2023-06-06T08:00:00","DSTA230108","Waiting spare",null,"No","No","No","Internal","Spare reed switch will be supplied at next convenient port."]

{"sheet":"Completed","index":1,"n_rows":347,"n_cols":28,"rows_kept":347,"cut":false,"hidden":false,"merged":[[10,8,10,9],[10,12,10,13],[12,6,12,27],[8,6,8,27]]}
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,"Defect - Damage Monitoring Sheet"]
[]
[null,null,null,null,null,null,null,"Date of Report","01-Jun-2023",null,null,"Ship Name","DHT STALLION (31-05-2023)"]
[]
[null,null,null,null,null,null,"VERSION : 2.0"]
[]
[]
[]
[null,null,null,"ID","SHIPSIDE UNIQUEID","UNIQUE ID","Date Recorded","Type of Deficiency","Observer code","Type of Inspection","Description of Deficiency","Equipment Categories","Area of Observation","Deficiency Cause","VIQ Ref Number","Risk Value of Obs","PSC Ref Number","PSC MOU ID","Action Taken or Required","Target Date","PO Ref No.","Status Code","Date Completed","Drydock","Info Sharing","Critical Item","Audit Type","Superintendent Remarks"]
[null,null,null,2606,null,"57_21/10/2019 9:30:28 AM","2019-03-04T23:59:35","Defect","Ship Staff","Ship Staff Insp.","No.1 Main LO pump seal leak.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Pump seal has been renewed.","2019-06-03T23:59:35","","Completed","2019-03-16T23:59:35","No","No","No","Internal"]
[null,null,null,2592,null,"57_20/10/2019 00:23:33","2019-05-02T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Axe was missing from the axe box on upper deck.","LSA / FFA","Safety / LSA / FFA","Inappropriate Procedure","5.43","High","","","Same to be put back.","2019-05-09T23:59:35","","Completed","2019-05-05T23:59:35","No","No","No","Internal"]
[null,null,null,2593,null,"57_20/10/2019 00:31:27","2019-05-02T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Aft Mooring winch gear oil sight glass is dirty and hence, oil level is not visible.","Deck - Mooring Machinery","Mooring","Equipment Related","10.25","Very High","","","Same to be cleaned","2019-06-02T23:59:35","","Completed","2019-05-07T23:59:35","No","No","No","Internal"]
[null,null,null,2595,null,"57_20/10/2019 9:24:10 AM","2019-05-02T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Mooring wire are found dry and muddy in appereance.","Deck - Mooring Machinery","Mooring","Behaviour Based","9.17","High","","","To be cleaned and greased.","2019-06-02T23:59:35","","Completed","2019-05-15T23:59:35","No","No","No","Internal"]
[null,null,null,2596,null,"57_20/10/2019 9:28:22 AM","2019-05-02T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Vent for emergency DG room cofferdam, is not stencilled.","Miscellaneous","Eng. / Strg. Comp.","Behaviour Based","11.17","Low","","","proper stenciling to be done.","2019-05-12T23:59:35","","Completed","2019-05-11T23:59:35","No","No","No","Internal"]
[null,null,null,2597,null,"57_20/10/2019 9:33:09 AM","2019-05-02T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Stencil for fire sensor at various locations are not proper.  Same is written by permanent marker","Miscellaneous","Emgcy. Systems","Behaviour Based","5.4","High","","","Proper stenciling to be done","2019-05-12T23:59:35","","Completed","2019-05-11T23:59:35","No","No","No","Internal"]
[null,null,null,2607,null,"57_21/10/2019 9:37:06 AM","2019-05-02T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Poster for “Alkaline and acidic chemicals to be kept separate” is missing in chemical locker.","Documentation,Miscellaneous","Eng. / Strg. Comp.","Inappropriate Procedure","10.29","Medium","","","Poster prepared and posted","2019-05-09T23:59:35","","Completed","2019-05-08T23:59:35","No","No","No","External"]
[null,null,null,2611,null,"57_21/10/2019 10:02:27 AM","2019-05-02T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","There is no protection / curtains for Aft hydraulics power panel, even though sea water line is passing near the starter panel. In forward store starter panel, arrangement is made but in aft it is missing.","Miscellaneous","Eng. / Strg. Comp.","Inappropriate Procedure","10.37","Medium","","","Plastic curtain and rod fabricated and fitted in place.","2019-08-02T23:59:35","","Completed","2019-05-23T23:59:35","No","No","No","External"]
[null,null,null,5614,null,"57_23/10/2019 9:40:25 AM","2019-05-02T23:59:35","Defect","Ship Staff","Suptd. Insp.","ME LO Purifier temeprature is set at 88'c. temperature to be maintained at 95'C","E/R - Purifier","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","All engineers briefed about the same.And temperature maintained at 95'C","2019-05-03T23:59:35","","Completed","2019-05-03T23:59:35","No","No","No","Internal"]
[null,null,null,2594,null,"57_20/10/2019 00:43:56","2019-05-04T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Aft hydraulic Mooring system, HP line flange in engine room(Boiler platform stbd side)  found having having leakage.","E/R - Pipes/ valves & fittings","Mooring","Equipment Related","10.29","Medium","","","HP pipe line O rings to be renewed and tested, no leakage.","2019-05-13T23:59:35","","Completed","2019-05-13T23:59:35","No","No","No","Internal"]
[null,null,null,2608,null,"57_21/10/2019 9:41:48 AM","2019-05-04T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Aft hydraulic mooring system, HP line flange in engine room ( boiler platform stbd side) found having leakage.","Deck - Mooring Machinery","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","HP pipe flange O-rings renewed and tested, no leaks observed.","2019-05-13T23:59:35","","Completed","2019-05-13T23:59:35","No","No","No","Internal"]
[null,null,null,2610,null,"57_21/10/2019 9:53:21 AM","2019-05-13T23:59:35","Defect","Ship Staff","Ship Staff Insp.","FWG Sea water inlet thermomter faulty","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Thermometer renewed","2019-05-23T23:59:35","","Completed","2019-05-18T23:59:35","No","No","No","Internal"]
[null,null,null,2612,null,"57_21/10/2019 10:11:12 AM","2019-05-13T23:59:35","Defect","Ship Staff","Ship Staff Insp.","ME Fuel oil auto filter element discs poor condition/some damaged and needs to be renewed.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","The correct filter elements supplied and replaced. ","2019-07-28T23:59:35","DSTA 190005/190056","Completed","2019-07-02T23:59:35","No","No","No","Internal"]
[null,null,null,2616,null,"57_21/10/2019 10:28:25 AM","2019-06-28T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","# 2 AE Lub oil priming pump motor - winding zero insulation","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","New motor received at S'pore on 01st Sept'19. Fitted on 04th Sept and tested, working satisfactory.","2019-09-03T23:59:35","GC's143E,167E / RO -DSTA 190097","Completed","2019-09-02T23:59:35","No","No","No","Internal"]
[null,null,null,2613,null,"57_21/10/2019 10:14:40 AM","2019-07-14T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","ME # 7 Unit PMI sensor cable accidentally cut","E/R - Main Engine","Eng. / Strg. Comp.","Human Error","10.32","Very High","","","New complete sensor with cable and connector received at S'pore on 01 sept 19, fitted, checked, found normal reading. ","2019-09-13T23:59:35","RO -DSTA 190098","Completed","2019-08-31T23:59:35","No","No","No","Internal"]
[null,null,null,2614,null,"57_21/10/2019 10:18:48 AM","2019-07-14T23:59:35","Defect","Ship Staff","Ship Staff Insp.","IG Scrubber area - Oxygen sensor defective /calibration not possible.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","New sensor received at S'pore on 01st New sensor received at S'pore on 01st Sept'19, fitted , calibrated and sensor reading normal.","2019-09-13T23:59:35","RO -DSTA 190062","Completed","2019-08-31T23:59:35","No","No","No","Internal"]
[null,null,null,7394,null,"57_13/12/2019 7:06:11 PM","2019-07-31T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Section 12 : Navigation lights and failure alarm not recorded during control test  in deck log book .\n\n\n\nWindow wiper are operational not recorded during control test  in deck log book .\n\n","Documentation","Navigation","Human Error","4.3","Medium","","","Same recorded in bridge note book. Refer to navigation procedures and navigation audit for entries to be made in bidge note book","2019-07-31T23:59:35","","Completed","2019-07-31T23:59:35","No","No","No","Internal"]
[null,null,null,7396,null,"57_13/12/2019 7:08:17 PM","2019-07-31T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Section 13 : The following were not recorded in the Bridge Note Book:\n\n\n\n•\tVerify berth to berth passage plan is available\n\n•\tVerify Under Keel Clearance calculations have been completed correctly for the time of departure\n\n•\tCheck charts for intended voyage are updated and available and courses plotted berth to berth\n\n","Documentation","Navigation","Human Error","4.1","High","","","Same recorded in bridge note book. Vessel will refer bridge note book and navigation audit checklist to make correct entries in bridge note book","2019-07-31T23:59:35","","Completed","2019-07-31T23:59:35","No","No","No","Internal"]
[null,null,null,2618,null,"57_21/10/2019 10:38:42 AM","2019-08-13T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","ME #2 unit FO Distributor block and aft fuel valve HP pipe threads damaged.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","New FO Distributor block with HP pipe and spares received & renewed. ","2019-09-13T23:59:35","RO-DSTA 195037","Completed","2019-09-07T23:59:35","No","No","No","Internal"]
[null,null,null,7379,null,"57_13/12/2019 11:37:04 AM","2019-08-14T23:59:35","Defect","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","The current edition of IMO publication 'IAMSAR Manual Volume III,\n\n2019 Edition - Mobil Facilities' was not available on board. The vessel had an old edition of\n\nIAMSAR Manual Vol. III 2016 Edition, but it didn't include the relevant amendments addressed\n\nin the MSC.1/Circ.1594 effective from 1 July 2019. A dispatch order from the vendor, dated 18\n\nJuly 2019, confirmed this publication had been booked.","Navigation - Others","Navigation","Human Error","4.12","Very High","","","New Edition was received at Rizhao, China.","2019-08-29T23:59:35","","Completed","2019-08-21T23:59:35","No","No","No","External"]
[null,null,null,7380,null,"57_13/12/2019 11:40:31 AM","2019-08-14T23:59:35","Defect","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","There were two oxygen sensors installed in the space containing the\n\ninert gas system in the engine room. However, it was noted the oxygen sensor positioned near\n\nthe inert gas scrubber unit was malfunctioning. Vessel had carried out the risk assessment and\n\nadditional pre-caution measures were in place.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","8.3","Very High","","","New sensors were received at Singapore on 01st Sep 2019 & replaced.","2019-09-13T23:59:35","","Completed","2019-08-30T23:59:35","No","No","No","External"]
[null,null,null,7381,null,"57_13/12/2019 11:44:14 AM","2019-08-14T23:59:35","Defect","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","Evidence of master's feedback for STS operations carried out in March\n\nand July 2019 was not available on board.","Miscellaneous","Navigation","Human Error","8.54","High","","","Master's feedback was prepared & previous records updated.","2019-08-18T23:59:35","","Completed","2019-08-16T23:59:35","No","No","No","External"]
[null,null,null,2615,null,"57_21/10/2019 10:25:08 AM","2019-08-25T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","ME # 2 FO Circulating pump - drive screw sheared","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Spare screw kit received at S'pore. Pump boxed back with new spares on 02nd Sept and tested on 03rd Sept. Found working satisfactory. ","2019-09-03T23:59:35","RO-DSTA 195041","Completed","2019-09-01T23:59:35","No","No","No","Internal"]
[null,null,null,2587,null,"57_18/10/2019 22:33:23","2019-08-30T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","Port side bridge wing camera not working.","Navigation - Others","Navigation","Equipment Related","4.7","High","","","Camera received on 13th Jan 2020 after repairs from shore and fitted on 14th Jan 2020","2020-01-30T23:59:35","","Completed","2020-01-12T23:59:35","No","No","No","Internal","Repair is in progress. Will be connected next call Singapore."]
[null,null,null,2591,null,"57_20/10/2019 10:15:53 AM","2019-08-30T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Fire Station wakie talkie -one pouch missing (3 pouches for 4 walkie talkies)","LSA / FFA","Communication","Behaviour Based,Human Error","5.43","High","","","Missing Pouch returned in place.","2019-09-06T23:59:35","","Completed","2019-09-01T23:59:35","No","No","No","Internal"]
[null,null,null,2598,null,"57_20/10/2019 10:21:17 AM","2019-08-30T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Bosun Store-Instruction regarding fire extinguisher fallen on floor.","LSA / FFA","Safety / LSA / FFA","Behaviour Based","5.42","Medium","","","Instruction for fire extinguisher inside bosun store put back in place","2019-09-02T23:59:35","","Completed","2019-09-01T23:59:35","No","No","No","Internal"]
[null,null,null,2599,null,"57_20/10/2019 10:26:21 AM","2019-08-30T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Fire extinguisher at entrance to cargo pump room-not checked in Aug 2019","LSA / FFA","Safety / LSA / FFA","Behaviour Based","5.42","Medium","","","Fire extinguisher at the entrance of pump room Inspected.","2019-09-06T23:59:35","","Completed","2019-09-05T23:59:35","No","No","No","Internal"]
[null,null,null,2600,null,"57_20/10/2019 10:29:51 AM","2019-08-30T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Deck foam line valve in foam room(Valve 13)  leaking from gland.","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.38","High","","","Foam line Valve No 13 Gland packing tightening well and it is rectified.","2019-09-06T23:59:35","","Completed","2019-09-05T23:59:35","No","No","No","Internal"]
[null,null,null,2601,null,"57_20/10/2019 10:36:29 AM","2019-08-30T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Deck foam pump inlet and outlet line pressurised(beacause  of sea water flushing valve leaking(","Deck - Pipe / Fittings","Safety / LSA / FFA","Equipment Related","5.38","High","","","Flushing globe valve gland packing opened and lapping of surface carried.  Found holding good.","2019-09-17T23:59:35","","Completed","2019-09-17T23:59:35","No","No","No","Internal"]
[null,null,null,2602,null,"57_20/10/2019 1:41:51 PM","2019-08-30T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Stbd Windlass brg dry.  Greasing to be carried out.","Deck - Mooring Machinery","Mooring","Behaviour Based","9.2","Very High","","","Greasing carried out before heaving up anchor at Fujairah.","2019-09-18T23:59:35","","Completed","2019-09-18T23:59:35","No","No","No","Internal"]
[null,null,null,2603,null,"57_20/10/2019 1:45:51 PM","2019-08-30T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Mooring Choke on sunken deck not stencilled.","Deck - Mooring Machinery","Mooring","Behaviour Based","9.19","Low","","","Completed stenciling","2019-09-17T23:59:35","","Completed","2019-09-17T23:59:35","No","No","No","Internal"]
[null,null,null,2604,null,"57_20/10/2019 1:49:38 PM","2019-08-30T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Port Windlass Gear Oil look emulisified.  Gear Oil to be renewed.","Deck - Mooring Machinery","Mooring","Equipment Related","9.2","Very High","","","Port Windlass Gear Oil drained, cleaned inside chamber and renewed with new Oil.","2019-10-13T23:59:35","","Completed","2019-10-03T23:59:35","No","No","No","Internal"]
[null,null,null,2605,null,"57_20/10/2019 1:52:23 PM","2019-08-30T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Cargo Stripping Pump Gland Packing Leaking","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.18","High","","","Cargo Stripping Pump gland Packing renewed.","2019-10-06T23:59:35","","Completed","2019-10-03T23:59:35","No","No","No","Internal"]
[null,null,null,2609,null,"57_21/10/2019 9:47:21 AM","2019-08-30T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","In ECR AMS, communication error alarm existing for master clock interface","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","As per message and instructions from Kamlesh, ROS 2 computer was restarted and alarm was reset / master clock synchronized.","2019-09-28T23:59:35","","Completed","2019-09-27T23:59:35","No","No","No","External"]
[null,null,null,2617,null,"57_21/10/2019 10:33:44 AM","2019-08-30T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ER vent fan control panel showing inverter alarm","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","We have checked the inverter panel for the fans and had also tried to put off and on the power. As such there is no alarm on the inverter. The alarms seen on the remote (ECR) panel are of 2018 and don't know why they are showing. ","2019-09-09T23:59:35","","Completed","2019-09-08T23:59:35","No","No","No","External"]
[null,null,null,2619,null,"57_21/10/2019 10:44:36 AM","2019-08-30T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Steam leakage from overhead pipe aft of ME system oil storage tank","Deck - Pipe / Fittings,E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Gaskets renewed and leakage rectified. ","2019-09-29T23:59:35","","Completed","2019-09-12T23:59:35","No","No","No","External"]
[null,null,null,2620,null,"57_21/10/2019 10:48:22 AM","2019-08-30T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","SCR decomposition unit inlet thermometer faulty.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Thermometer renewed.","2019-09-28T23:59:35","","Completed","2019-09-19T23:59:35","No","No","No","External"]
[null,null,null,2621,null,"57_21/10/2019 10:52:00 AM","2019-08-30T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","220V low insulation- Insulation level at 2M ohm when deck lights are switched on.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","The low insulation was originating from the forward navigation light, same has been repaired and fault rectified. ","2019-09-28T23:59:35","","Completed","2019-09-25T23:59:35","No","No","No","External"]
[null,null,null,7382,null,"57_13/12/2019 1:32:07 PM","2019-08-30T23:59:35","Non Conformity","Owner / Marine / Tech. Suptd.","ISPS Audit","Gangway briefing for visitors was not done as per Goodwood best practice","Documentation","ISPS Related","Human Error","5.47","Medium","","","All crew briefed about the importance for safety and secuiry requirements  by keeping proper gangway watches.","2019-09-29T23:59:35","","Completed","2019-09-06T23:59:35","No","No","No","Internal"]
[null,null,null,7383,null,"57_13/12/2019 1:35:16 PM","2019-08-30T23:59:35","Non Conformity","Owner / Marine / Tech. Suptd.","ISM Audit","Ships ensign flag was not flown on the stern ","Miscellaneous","ISM Related","Human Error","5.47","Medium","","","All crewmembers briefed. Duty AB and Duty officer during take over to verify that the flags are properly deployed.","2019-09-29T23:59:35","","Completed","2019-09-06T23:59:35","No","No","No","Internal"]
[null,null,null,7384,null,"57_13/12/2019 1:38:12 PM","2019-08-30T23:59:35","Defect","Owner / Marine / Tech. Suptd.","ISM Audit","Life vest was not provided prior entry on the Billy Pug","Miscellaneous","ISM Related","Human Error","5.47","Medium","","","Life vest to  be kept tied on the personal transfer basket for immediate use. Crew briefing carried out, and duty officer  in charge and bosun to verify the same before lowering the basket.","2019-09-29T23:59:35","","Completed","2019-09-01T23:59:35","No","No","No","Internal"]
[null,null,null,7385,null,"57_13/12/2019 1:41:44 PM","2019-08-30T23:59:35","Defect","Owner / Marine / Tech. Suptd.","ISM Audit","Gangway placard - no smart watches permitted - is not stenciled","Miscellaneous","ISM Related","Inappropriate Procedure","5.47","Medium","","","All required information to be stenciled on the notice board, as per HSQEEn requiremnt. Crew briefed about the safety requirement needed on deck , and the consequence of a hazard if using smart watches on deck.  Any information required to be displayed should be stenciled as soon as possible with out delay.","2019-09-29T23:59:35","","Completed","2019-09-05T23:59:35","No","No","No","Internal"]
[null,null,null,7386,null,"57_13/12/2019 1:50:20 PM","2019-08-30T23:59:35","Non Conformity","Owner / Marine / Tech. Suptd.","ISM Audit","2 scuppers (stbd aft main deck) & i.w.o. 3 (S) COT were found un-shipped during bunker operations ","Hull & Tanks","MARPOL Related","Human Error","6.2","High","","","Scuppers to be plugged well before arrival, port and only the aft 2 scuppers to be left open for rain water to drain before arrival.  As crew will be busy after arrival port, this will save time. Duty officers to verify, and at least  2 persons to visually  to confirm and report that the scuppers are in place.","2019-09-29T23:59:35","","Completed","2019-09-06T23:59:35","No","No","No","Internal"]
[null,null,null,7387,null,"57_13/12/2019 1:53:14 PM","2019-08-30T23:59:35","Non Conformity","Owner / Marine / Tech. Suptd.","ISM Audit","Vessel equipped with fixed piping to manage oil spills on main deck. But fuel tank air pipes are located aft main deck - with no facilities to contain a spill ","Miscellaneous","MARPOL Related","Human Error","6.3","Low","","","During bunkering time, seperate portable wilden pump to be rigged aft of the fish plate to tackle , spillls from bunker tank vents. Duty officer and person incharge of the operation to verify portable wilden pump is rigged before the bunkering starts.","2019-09-29T23:59:35","","Completed","2019-09-06T23:59:35","No","No","No","Internal"]
[null,null,null,7388,null,"57_13/12/2019 5:45:13 PM","2019-08-30T23:59:35","Defect","Owner / Marine / Tech. Suptd.","ISM Audit","Minor Hydraulic leak was sighted forward of P/R entrance ","Cargo Mach.","Cargo / Ballast Systems","External Factors","6.3","Low","","","Any leakages on deck to be rectified as soon as possible, and the area to be cleaned prior arrival port.Leakages to be checked and ientified during the safety rounds and repairs to be carried out as soon as possible before arrival port.","2019-09-29T23:59:35","","Completed","2019-09-07T23:59:35","No","No","No","Internal"]
[null,null,null,7389,null,"57_13/12/2019 5:49:24 PM","2019-08-30T23:59:35","Defect","Owner / Marine / Tech. Suptd.","ISM Audit","Port anchor hawse pipe - cover was not firmly fixed. It was easily opened with just one tug as the locking pins were not secured ","Hull & Tanks","General Appearance","Human Error","7.12","High","","","Crew and officers briefed, and the requirement of closing the anchor hawse pipe to prevent robbery discussed. After dropping anchor each time, crew to cover the anchor hawse pipe cover properly and Chief officer to verfiy and report. ","2019-09-29T23:59:35","","Completed","2019-09-07T23:59:35","No","No","No","Internal"]
[null,null,null,7390,null,"57_13/12/2019 6:51:00 PM","2019-08-30T23:59:35","Non Conformity","Owner / Marine / Tech. Suptd.","Engineering Audit","In ECR - alarm monitoring system - MSBD abnormal alarm found off scan ","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Knowledge Based","10.2","Low","","","MSBD alarm offscan disabled and all engineers briefed on the consequences.All engineers were briefed about importances of certain alarms and consequences in offscanning of alarms. Without chief engineer permission no alarms to be offscanned or disabled. ","2019-09-29T23:59:35","","Completed","2019-08-30T23:59:35","No","No","No","Internal"]
[null,null,null,5599,null,"57_23/10/2019 9:55:21 AM","2019-08-30T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","LO drums were lifted without using safety lead to control swing. Crew to be briefed\t\t","Miscellaneous","Crew Management","Human Error,Inappropriate Procedure","5.11","Low","","","All crew briefed during toolbox meeting after  departure port","2019-09-06T23:59:35","","Completed","2019-09-02T23:59:35","No","No","No","Internal"]
[null,null,null,7391,null,"57_13/12/2019 6:54:36 PM","2019-08-30T23:59:35","Defect","Owner / Marine / Tech. Suptd.","ISM Audit","LO drums were lifted without using safety lead to control swing","Miscellaneous","Crew Management","Human Error","5.11","Low","","","Crew to be tie at least two lead line to prevent the swing on the drum  And thus preventing the wild swing. Crew briefed and trained, specially for these jobs. Supervision of the job  by officer incharge, and immedeate stop work procedure incase of any wrong action.","2019-09-29T23:59:35","","Completed","2019-09-01T23:59:35","No","No","No","Internal"]
[null,null,null,5600,null,"57_23/10/2019 9:58:29 AM","2019-08-30T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Small steels pipes in ER workshop not lashed\t","Miscellaneous","Eng. / Strg. Comp.","Behaviour Based,Inappropriate Procedure","5.11","Low","","","small steel pipes etc removed ,placed properly and lashed.","2019-09-02T23:59:35","","Completed","2019-09-01T23:59:35","No","No","No","Internal"]
[null,null,null,5601,null,"57_23/10/2019 10:02:42 AM","2019-08-30T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Grey water pump leaking from flange\t","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","gasket changed, save all trays painted","2019-09-06T23:59:35","","Completed","2019-09-05T23:59:35","No","No","No","Internal"]
[null,null,null,7393,null,"57_13/12/2019 7:02:04 PM","2019-08-30T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Nav Audit / Verification","Masters's signature on flwg were not available from 21 Aug. Deck log book, Bell book , GMDSS log books\n\n","Documentation","Cert. & Docu.","Human Error","4.23","High","","","All officers briefed, regarding the strict requirement of keeping bridge watches and handing over requirement.All officers to complete their log book and sign and relieving officer to check, and report to master.  Master  & chief officer to check and verify  and complete log books for the previous day .","2019-10-30T23:59:35","","Completed","2019-09-14T23:59:35","No","No","No","Internal"]
[null,null,null,5602,null,"57_23/10/2019 10:38:44 AM","2019-08-30T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","IG system fresh air intake flange wing nuts to ease up\t","Inert Gas","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Wing nuts eased up and greased","2019-09-06T23:59:35","","Completed","2019-09-06T23:59:35","No","No","No","Internal"]
[null,null,null,5603,null,"57_23/10/2019 10:42:18 AM","2019-08-30T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp."," MGO filling line safety valve opening pressure not stencilled\t\t\t\t\t\t\t\t","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Behaviour Based,Equipment Related","10.8","Medium","","","opening pressure stencilled- 5.0bar","2019-09-06T23:59:35","","Completed","2019-09-01T23:59:35","No","No","No","Internal"]
[null,null,null,5604,null,"57_23/10/2019 10:45:07 AM","2019-08-30T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Lifting hooks in steering gear room\t","Miscellaneous","Eng. / Strg. Comp.","Inappropriate Procedure","10.28","Low","","","all hooks color coded and SWL color code laminated poster posted in steering gear room","2019-09-16T23:59:35","","Completed","2019-09-16T23:59:35","No","No","No","Internal"]
[null,null,null,5605,null,"57_23/10/2019 11:34:13 AM","2019-08-30T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Main engine attached hydraulic pump no:3 accumulator cap has fallen down\t","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Cap fitted back","2019-09-28T23:59:35","","Completed","2019-09-23T23:59:35","No","No","No","Internal"]
[null,null,null,5606,null,"57_23/10/2019 11:37:34 AM","2019-08-30T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Rudder rams (P fwd & Aft) have more leakage than stbd ones\t","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Packing gland tightened as per maker instructions, oil leak reduced, under observation","2019-09-29T23:59:35","","Completed","2019-09-23T23:59:35","No","No","No","Internal"]
[null,null,null,5607,null,"57_23/10/2019 11:40:32 AM","2019-08-30T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","In ECR ams, communication error alarm existing for master clock interface\t\t","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","As per msg from Suptd. Kamlesh, ROS2 computer restarted annd alarm was reset. Master clock interface working in order.","2019-09-28T23:59:35","","Completed","2019-09-29T23:59:35","No","No","No","Internal"]
[null,null,null,5608,null,"57_23/10/2019 11:43:39 AM","2019-08-30T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Spare hydraulic motors for windlass and winch kept in steering gear room to identify and also update in PAL PMS\t","Miscellaneous","Eng. / Strg. Comp.","Behaviour Based","5.11","Low","","","Spare motors shifed to mid ship locker and location in PAL updated","2019-09-29T23:59:35","","Completed","2019-10-12T23:59:35","No","No","No","Internal"]
[null,null,null,5615,null,"57_23/10/2019 9:46:54 AM","2019-08-30T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","In ECR Alarm monitoring system \"MSBD abnormal\" alarm found offscan\t\t\t\t","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Behaviour Based,Equipment Related","10.38","Medium","","","Removed from offscan, alarm reset","2019-08-31T23:59:35","","Completed","2019-08-30T23:59:35","No","No","No","Internal"]
[null,null,null,5616,null,"57_23/10/2019 11:46:19 AM","2019-08-30T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","C2E feed pump discharge pressure guage needle broken\t","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.31","Very High","","","pressure guage renewed with spare","2019-10-06T23:59:35","","Completed","2019-10-13T23:59:35","No","No","No","Internal"]
[null,null,null,7392,null,"57_13/12/2019 6:58:23 PM","2019-09-03T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Poor quality Squid supplied by ship chandellor ","Accommodation","MLC Related","External Factors","","","","","If bad quality items supplied, immedeately return back the items, and report the matter to company.Prior instructions to be given, to ship chandler, that if any  items are found ito be in a bad condition, it will be rejected and  returned by the same boat.","2019-09-18T23:59:35","","Completed","2019-09-13T23:59:35","No","No","No","Internal"]
[null,null,null,2588,null,"57_20/10/2019 4:51:03 PM","2019-09-10T23:59:35","Defect","Ship Staff","Ship Staff Insp.","BWTS No 1 Loop Filter inlet valve BA 614 & No1 loop filter Bypass valve BA 616 suspect valve passing in closed position.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","6.21","High","","","Both Vaves were observed for integrity during ballasting operation at PAL, USWC and confimred to be holding. Will monitor again during Ballast exchange prior arrival Loadport.","2019-12-09T23:59:35","","Completed","2019-11-07T23:59:35","No","No","No","Internal","Vessel is supplied with spare seat rings for ballast line. Renew seat rings if valves are leaking."]
[null,null,null,2590,null,"57_18/10/2019 22:47:02","2019-09-10T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Ballast valves BA508 & BA510 is kept at 20% open to prevent the valve to be stuck at closed position.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.11","Medium","","","Both the valves renewed & tested. Working satisfactorily.","2019-12-09T23:59:35","DSTA-190089","Completed","2019-10-11T23:59:35","No","No","No","Internal"]
[null,null,null,7400,null,"57_13/12/2019 12:58:05 PM","2019-11-04T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Nav Audit / Verification","Echo sounder scale in Use not mentioned for Departure Rastanura on 26th Sept 2019.","Documentation","Navigation","Human Error","4.19","Low","","","Appropriate entries made & observation has been closed out.","2020-02-04T23:59:35","","Completed","2019-11-10T23:59:35","No","No","No","Internal"]
[null,null,null,7401,null,"57_13/12/2019 1:03:06 PM","2019-11-04T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Nav Audit / Verification","Company Standing Orders and Master's Standing Orders not countersigned by Watch keeping Ratings.","Documentation","Navigation","Human Error","4.1","High","","","Ratings were briefed regarding the requirement. Master's & Company Standing orders were countersigned by Watch ratings & observation closed out. ","2020-02-04T23:59:35","","Completed","2019-11-11T23:59:35","No","No","No","Internal"]
[null,null,null,7402,null,"57_13/12/2019 1:05:58 PM","2019-11-04T23:59:35","Defect","Owner / Marine / Tech. Suptd.","ISPS Audit","Gangway log not properly filled up for Visitor card numbers at Rastanura.","Documentation","ISPS Related","Human Error","7.12","High","","","Approrpiate entries were made & observation closed out. Crew briefing carried out to prevent recurrence.","2020-02-04T23:59:35","","Completed","2019-11-13T23:59:35","No","No","No","Internal"]
[null,null,null,7403,null,"57_13/12/2019 1:14:45 PM","2019-11-04T23:59:35","Defect","Owner / Marine / Tech. Suptd.","ISM Audit","Cargo tank valve operation log for loading at Rastanura not completed.","Documentation","Cargo / Ballast Systems","Human Error","8.12","Medium","","","Cargo tank valve operation log was completed. Officers were given training to prevent recurrence.","2020-02-04T23:59:35","","Completed","2019-11-11T23:59:35","No","No","No","Internal"]
[null,null,null,7404,null,"57_13/12/2019 1:16:33 PM","2019-11-04T23:59:35","Non Conformity","Owner / Marine / Tech. Suptd.","ISM Audit","Toolbox meeting section for “Days jobs completed to Satisfaction and Verified by” not signed by Concerned officer from 15th Oct 2019 to 01st Nov 2019","Documentation","ISM Related","Human Error","5.2","Very High","","","Required entries made & NC closed out. Training conducted to prevent recurrence.","2020-02-04T23:59:35","","Completed","2019-11-18T23:59:35","No","No","No","Internal"]
[null,null,null,7405,null,"57_13/12/2019 1:25:14 PM","2019-11-04T23:59:35","Defect","Owner / Marine / Tech. Suptd.","ISM Audit","Vessel was carrying High H2S Cargo however “Precautions when carrying High H2S Cargoes” was not posted in Common spaces of Accommodation.","Documentation","ISM Related","Human Error","5.47","Medium","","","Required Poster prepared and put up at Various locations.","2020-02-04T23:59:35","","Completed","2019-11-12T23:59:35","No","No","No","Internal"]
[null,null,null,7406,null,"57_13/12/2019 1:08:09 PM","2019-11-04T23:59:35","Defect","Owner / Marine / Tech. Suptd.","MLC Audit","Knives used for cutting Meat and Vegetables are not Color coded as per the Color code chart in the Galley.","Accommodation","MLC Related","Knowledge Based","11.13","Low","","","Color coding done for various knives and observation closed out.","2020-02-04T23:59:35","","Completed","2019-11-13T23:59:35","No","No","No","Internal"]
[null,null,null,7407,null,"57_13/12/2019 1:18:41 PM","2019-11-04T23:59:35","Defect","Owner / Marine / Tech. Suptd.","ISM Audit","Flame screen of 2S P/V Valve (Vacuum side) dislodged from the frame on one side.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.19","High","","","Dislodged section of Flame Screen fitted back in position & observation closed out.  ","2020-02-04T23:59:35","","Completed","2019-11-14T23:59:35","No","No","No","Internal"]
[null,null,null,7408,null,"57_13/12/2019 1:11:39 PM","2019-11-04T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Engineering Audit","Scope of Implementation starting date for 10) Propeller maintenance (Cleaning / Polishing) not mentioned in the Action Plan","Documentation","Cert. & Docu.","Inappropriate Procedure","10.12","Very High","","","Action plan amended and observation closed out.","2020-02-04T23:59:35","","Completed","2019-11-10T23:59:35","No","No","No","Internal"]
[null,null,null,7409,null,"57_13/12/2019 1:22:26 PM","2019-11-04T23:59:35","Defect","Owner / Marine / Tech. Suptd.","ISM Audit","No locking or sealing arrangement is provided for Galley comminutor.","Accommodation","MARPOL Related","Inappropriate Procedure","6.2","High","",""," locking arrangement made, poster pasted near the commuter. also breaker will be kept off in port.","2020-02-04T23:59:35","","Completed","2020-01-04T23:59:35","No","No","No","Internal"]
[null,null,null,5610,null,"57_23/10/2019 11:48:48 AM","2019-11-06T23:59:35","Breakdown,Defect","Ship Staff","Ship Staff Insp.","Steering gear rudder carrier greasing pump body cracked","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Spares received at singapore on 13/01/2020. New grease pump fitted, working staisfactory.","2020-02-10T23:59:35","DSTA190159","Completed","2020-01-23T23:59:35","No","No","No","Internal","Spare is ready for supply. Waiting for convenient port. Revise target date as spare can be supplied at Singapore only."]
[null,null,null,6285,null,"57_20/11/2019 2:33:15 PM","2019-11-10T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","Experiencing issues with Bridge Window Wiper controller panel. At present, the following wipers are in-operational :\n\nWiper No.1 \n\nWiper No.3 \n\nWiper No.5\n\nWiper No.6\n\nWiper No.7\n\nWiper No.9","Navigation - Others","Navigation","Equipment Related","4.7","High","","","New controller panel and senser received and fitted. system working satisfactory","2020-02-09T23:59:35","DSTA190174","Completed","2020-01-13T23:59:35","No","No","No","Internal","Spare will be ready on 10th Jan. Will be connected accordingly."]
[null,null,null,6286,null,"57_20/11/2019 11:06:06 PM","2019-11-10T23:59:35","Other","Owner / Marine / Tech. Suptd.","Ship Staff Insp.","Job operational spares to be updated in PAL.","Miscellaneous","Cert. & Docu.","Inappropriate Procedure","10.12","Very High","","","Job Operational spares to be updated in PAL.","2020-01-23T23:59:35","","Completed","2020-01-08T23:59:35","No","No","No","Internal","Complete this job ASAP."]
[null,null,null,7395,null,"57_13/12/2019 7:19:23 PM","2019-11-17T23:59:35","Defect","Owner / Marine / Tech. Suptd.","ISM Audit","12.20.05.011.04 Pre Arrival and commencement of cargo Operation checklist for loading at Juaymah - Section B (To be completed 24 Hrs prior operation) completed on 21 Sept 2019 at 1500 LT while loading operation commenced on 24 Sept 2019 1325 Hrs. ","Documentation","Cargo / Ballast Systems","Human Error","2.3","High","","","Required entries made & observation has been closed out.","2019-12-17T23:59:35","","Completed","2019-11-30T23:59:35","No","No","No","Internal"]
[null,null,null,7397,null,"57_13/12/2019 7:29:03 PM","2019-11-17T23:59:35","Defect","Owner / Marine / Tech. Suptd.","ISM Audit","CCR Movement Log : Entry for Independent check of Line up did not include Venting prior Loading operation at Juaymah on 24 Sept 2019.","Documentation","ISM Related","Human Error","2.3","High","","","Required entries made & observation has been closed out.","2019-12-17T23:59:35","","Completed","2019-11-30T23:59:35","No","No","No","Internal"]
[null,null,null,7398,null,"57_13/12/2019 7:31:23 PM","2019-11-17T23:59:35","Defect","Owner / Marine / Tech. Suptd.","ISM Audit","Pre Arrival Tests and Checks prior Loading at Juaymah did not include any test and checks for BWTS system.","Documentation","ISM Related","Human Error","2.3","High","","","Required entries made & observation has been closed out.","2019-12-17T23:59:35","","Completed","2019-11-30T23:59:35","No","No","No","Internal"]
[null,null,null,7399,null,"57_13/12/2019 7:34:04 PM","2019-11-17T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Bunkering Audit","Bunker Transfer Plan / Checklist 12.04.08.011.01 Section 7 - Monitoring of H2S/Benzene Vapors : \n\nBenzene reading measured by detector tubes shall be mentioned < Min value that can be measured by the specific tube. For example by Gastec tubes Min measurable value is 0.05 ppm, hence in that case benzene shall be mention <0.05 ppm (if no discoloration observed)\n\nUnderstand vessel has kept the Gas tubes as evidence of monitoring.\n\n","Documentation","ISM Related","Human Error","10.8","Medium","","","Required entires made & observation has been closed out.","2019-12-17T23:59:35","","Completed","2019-11-30T23:59:35","No","No","No","Internal"]
[null,null,null,5609,null,"57_22/10/2019 2:23:29 PM","2019-11-20T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Cargo Oil tank Pressure Sensor for 1 Port tank and 4 Stbd Showing erratic","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.13","Medium","","","1P Pressure sensor renewed with spare sensor available onboard and is presently under observation.                                                           Cargo tank Pressure sensor for 4S renewed with new spare. working satisfactory.","2020-02-19T23:59:35","DSTA190156","Completed","2020-01-19T23:59:35","No","No","No","Internal","3 nos, spare sensors are on order, for vessel to keep 1 as spare. Will be connected next call Singapore."]
[null,null,null,5611,null,"57_27/10/2019 8:15:30 AM","2019-11-22T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Red warning  light Glass  Shade for Hose handling crane Port side broken","Deck - Machinery,Elect. Mach. & Equip.","Emgcy. Systems","Equipment Related","8.63","High","","","Complete new fitting with glass receive at singapore on 13/01/2020. Working satisfactory.","2020-02-21T23:59:35","DSTA-190163","Completed","2020-01-19T23:59:35","No","No","No","Internal","Liaise with procure - give details of spare required and maker."]
[null,null,null,6284,null,"57_Fri Jan 11 2019 05:50:52 GMT+0000 (Coordinated Universal Time)","2019-11-28T23:59:35","Breakdown,Defect","Ship Staff","Ship Staff Insp.","Fwd Anchor light and fitting damaged","Navigation - Others","Navigation","Equipment Related,External Factors","4.8","Medium","","","Fwd Anchor light fitting replaced and tried satisfactorily ","2020-03-29T23:59:35","DSTA190166","Completed","2020-03-08T23:59:35","No","No","No","Internal"]
[null,null,null,7410,null,"57_15/12/2019 10:19:36 AM","2019-12-16T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Navigation light failure alarm for Port Main Side light is in-operative.","Navigation - Others","Navigation","Equipment Related","4.3","Medium","","","Navigation Alarm PCB replaced and alarm tried out satisfactorily ","2020-03-29T23:59:35","DSTA-190157","Completed","2020-03-08T23:59:35","No","No","No","Internal","Spare will be ready by 1st Jan 2020. Will be connected while passing Singapore."]
[null,null,null,9054,null,"57_26/12/2019 4:31:04 AM","2019-12-19T23:59:35","Defect","Ship Staff","Ship Staff Insp.","DG Viscotherm showing wrong values","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.1","Medium","","","Sensor received and replaced, working - satisfactory","2020-01-29T23:59:35","Spare requested on excel sheet","Completed","2020-01-18T23:59:35","No","No","No","Internal","PO under process. Getting quotation from various suppliers."]
[null,null,null,9868,null,"57_11/1/2020 7:09:25 AM","2019-12-31T23:59:35","Defect","Ship Staff","Ship Staff Insp.","BWTS c2e unit flow meter 952 is defective.","E/R - Aux. Mach.","Cargo / Ballast Systems","Equipment Related","6.22","Medium","","","Fow meter 952 found choked with salt deposits. cleaned and tried out found working satisfactory","2020-03-29T23:59:35","DSTA200009","Completed","2020-03-29T23:59:35","No","No","No","Internal"]
[null,null,null,9869,null,"57_11/1/2020 7:33:22 AM","2020-01-03T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Engine room store packeged A/C pressure switch is defective.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.1","Medium","","","pressure switch replaced with new one.","2020-02-26T23:59:35","DSTA200017","Completed","2020-02-03T23:59:35","No","No","No","Internal"]
[null,null,null,10405,null,"57_28/1/2020 10:50:54 AM","2020-01-17T23:59:35","Defect","Ship Staff","Ship Staff Insp.","ME unit no.7 second piston ring broken at butt area(app.40mm)","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.1","Medium","","","ME unit#7 all piston rings renewed by service engineer with shore staff.","2020-02-26T23:59:35","","Completed","2020-01-31T23:59:35","No","No","No","Internal"]
[null,null,null,10451,null,"57_Wed Feb 12 2020 10:29:02 GMT+0000","2020-01-31T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Temperature log sheet for CO2 cylinder for Emergency DG room missing.","LSA / FFA","Safety / LSA / FFA","Inappropriate Procedure","5.35","Medium","","","temperature log sheet put in place and updated on weekly basis.","2020-02-26T23:59:35","","Completed","2020-02-03T23:59:35","No","No","No","Internal"]
[null,null,null,10452,null,"57_Wed Feb 12 2020 10:33:55 GMT+0000","2020-01-31T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Quick closing valve for emergency DG operating box rusted.","LSA / FFA","General Appearance","Equipment Related","10.17","Very High","","","Box derusted and painted.","2020-02-27T23:59:35","","Completed","2020-02-03T23:59:35","No","No","No","Internal"]
[null,null,null,10453,null,"57_Wed Feb 12 2020 10:46:57 GMT+0000","2020-01-31T23:59:35","Non Conformity","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Restricted area not tagged. Tags not found in emergency DG room, CO2 room and various other restricted area.","LSA / FFA","ISPS Related","Inappropriate Procedure","7.5","Low","","","All restricted area  identified and tagged.","2020-02-27T23:59:35","","Completed","2020-02-04T23:59:35","No","No","No","Internal"]
[null,null,null,10454,null,"57_Wed Feb 12 2020 11:05:14 GMT+0000","2020-01-31T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Various dampers in ME exhaust line to grease","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Greasing carried out as per lube oil chart, renolit lx-pep 2/3.","2020-03-29T23:59:35","","Completed","2020-02-14T23:59:35","No","No","No","Internal"]
[null,null,null,10455,null,"57_Wed Feb 12 2020 11:23:19 GMT+0000","2020-01-31T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Engine room vent fan control panel in alarm condition.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Spare cooling fans received renewed for ER supply fan no 1 and 4. Now working satisfactory and no alarm indication is present. Job order no: V-DSTA020980/21, V-DSTA020979/21","2021-02-26T23:59:35","","Completed","2021-01-27T23:59:35","No","No","No","Internal","Spare is ready for supply."]
[null,null,null,10475,null,"57_Sat Feb 15 2020 09:27:07 GMT+0000","2020-01-31T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Main Engine LO purifier operating at 81 deg C","E/R - Purifier","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","LO purifier temperature increased to 94 degree and same instructed to ship staff.","2020-02-18T23:59:35","","Completed","2020-01-31T23:59:35","No","No","No","Internal"]
[null,null,null,10476,null,"57_Sat Feb 15 2020 09:30:58 GMT+0000","2020-01-31T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Sewage Treatment Plant re-circulation flow not visible.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","transparent pipe replaced with new one, line cleared. now flow is clearly visible.","2020-02-27T23:59:35","","Completed","2020-02-04T23:59:35","No","No","No","Internal"]
[null,null,null,10477,null,"57_Sat Feb 15 2020 09:34:01 GMT+0000","2020-01-31T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","220V insulation at 10 M ohm.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.38","Medium","","","low insulation was coming from service air dryer drain solenoid valve same rectified.","2020-02-27T23:59:35","","Completed","2020-02-08T23:59:35","No","No","No","Internal"]
[null,null,null,10478,null,"57_Sat Feb 15 2020 09:37:19 GMT+0000","2020-01-31T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","3C, 4S, 3S cargo tank dome packing to renew.","Hull & Tanks","Cargo / Ballast Systems","Equipment Related","2.16","Medium","","","All butterfly nuts were unevenly tightened; currently no leaks after nuts were evenly tightened","2020-03-29T23:59:35","","Completed","2020-02-06T23:59:35","No","No","No","Internal"]
[null,null,null,10479,null,"57_Sat Feb 15 2020 09:42:44 GMT+0000","2020-01-31T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Windlass stbd and port gear oil emulsified.","Deck - Mooring Machinery","Mooring","Equipment Related","9.2","Very High","","","Gear oil renewed in WI (Stbd windlass). W2 (Port windlass) oil found in good condition","2020-03-29T23:59:35","","Completed","2020-04-05T23:59:35","No","No","No","Internal"]
[null,null,null,10480,null,"57_Sat Feb 15 2020 09:44:39 GMT+0000","2020-01-31T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Brake clearance to check and adjust for all Winches and Windlass.","Deck - Mooring Machinery","Mooring","Equipment Related","9.15","Medium","","","All Winches Brake Adjustment check nuts adjusted and freed as required ","2020-03-29T23:59:35","","Completed","2020-03-05T23:59:35","No","No","No","Internal"]
[null,null,null,11438,null,"57_27/3/2020 11:49:36 PM","2020-03-25T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Main engine Unit #6 piston rings found having scuffing and middle piston ring found broken at the end","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","ME Unit #6 Piston rings renewed with cermet coated rings , Cylinder liner renewed by shore team. Investigation carried out by MAN technician, HSD and ship staff for the scuffing.Corrective and preventive actions taken as advised.","2020-04-03T23:59:35","","Completed","2020-04-03T23:59:35","No","No","No","Internal"]
[null,null,null,11437,null,"57_16/4/2020 2:42:42 PM","2020-04-04T23:59:35","Critical Equipment","Ship Staff","Ship Staff Insp.","Cargo OB discharge v/v CL-151 (solenoid fitting in R/Rm) has to be manually moved once command (for OPEN/SHUT) given by the ODME panel","Critical Equip.","Eng. / Strg. Comp.","Equipment Related","6.13","Low","","","New Flowmeter with Open/Shut limit switch requistioned - awaiting spares. Time being the system can be operated but one person needs to stby at the solenoid box while ODME is tested/operational","2020-07-29T23:59:35","DSTA200099","Completed","2020-07-07T23:59:35","No","No","No","Internal","Spare will be supplied at Singapore on 2nd July."]
[null,null,null,11608,null,"57_30/4/2020 4:01:13 AM","2020-04-18T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","BWTS SYSTEM- Minor leak from anolyte pump","E/R - Pumps","Cargo / Ballast Systems","Equipment Related","10.29","Medium","","","Leak rectified","2020-10-29T23:59:35","","Completed","2020-09-01T23:59:35","No","No","No","Internal","Please mention RO no or  GC no . Target date revised."]
[null,null,null,11609,null,"57_30/4/2020 2:35:43 AM","2020-04-18T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Cold repair on STBD life boat cooling water tank","LSA / FFA","Emgcy. Systems","Equipment Related","10.31","Very High","","","The cracked/ damaged exhaust manifold pipe replaced with spare new one. Engine tried out staisfactory.","2021-02-26T23:59:35","","Completed","2021-01-26T23:59:35","No","No","No","Internal","Spare is ready at Singapore. Will be supplied while passing Singapore."]
[null,null,null,11610,null,"57_30/4/2020 4:45:36 AM","2020-04-18T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","No.1 Main LO pump- Lip seal leaking","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Seal renewed , same found leaking again. JOB PENDING. Seal leak checked in port and found very slight oil leaks when pump is in operation need seal sleeve renewal","2021-03-29T23:59:35","DSTA200084","Completed","2020-06-17T23:59:35","No","No","No","Internal","Check LO return pipe as advised by maker."]
[null,null,null,11611,null,"57_30/4/2020 10:14:52 PM","2020-04-18T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Out of 32 COT hatches - Rubber packing for 19 were renewed due to leaks. Remaining 13 COT hatches not leaking but suggest to change at 1st oppurtunity","Hull & Tanks","Cargo / Ballast Systems","Equipment Related","8.21","High","","","Spares received,renewal of leaking cargo tankdome rubber packing completed","2020-10-29T23:59:35","DSTA200111","Completed","2020-08-23T23:59:35","No","No","No","Internal","Job in progress. Target date revised."]
[null,null,null,11612,null,"57_23/4/2020 11:53:21 PM","2020-04-18T23:59:35","Critical Equipment","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ODME  ovbd valve  CL151 valve block indicator not working","Critical Equip.","Cargo / Ballast Systems","Equipment Related","6.13","Low","","","Defective spare part to be renewed.","2020-08-16T23:59:35","","Completed","2020-07-07T23:59:35","No","No","No","Internal"]
[null,null,null,11613,null,"57_30/4/2020 10:24:38 PM","2020-04-18T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Pipes fretting due to vibration","Deck - Pipe / Fittings","Cargo / Ballast Systems","Industry Issue","8.1","Very High","","","Teflon padding to put to prevent fretting damage to pipes at two locations","2020-10-29T23:59:35","","Completed","2020-09-13T23:59:35","No","No","No","Internal","When expected to complete?"]
[null,null,null,11614,null,"57_23/4/2020 11:33:34 PM","2020-04-18T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Engine bell book recording not as per check list 12.01.10.021.00","Documentation","Cert. & Docu.","Human Error","10.5","Low","","","Follow instruction strictly as per 12.01.10.021.00. Record starting/stopping additional DG etc","2020-05-03T23:59:35","","Completed","2020-04-18T23:59:35","No","No","No","Internal"]
[null,null,null,11615,null,"57_24/4/2020 12:03:49 AM","2020-04-18T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","CE night order book -Last entry was 11 March. No instruction found for last cargo discharge/arrival/dep discharge port etc","Miscellaneous","Cert. & Docu.","Behaviour Based,Human Error","10.5","Low","","","Started writing night order book regularly to comply with VIQ requirements","2020-05-03T23:59:35","","Completed","2020-04-18T23:59:35","No","No","No","Internal"]
[null,null,null,11616,null,"57_30/4/2020 2:42:07 AM","2020-04-18T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","CO2 System for Emcy Gen Room- CO2 bottles found rusted at bottom","LSA / FFA","Emgcy. Systems","Equipment Related","10.1","Medium","","","CO2 bottles derusted and painted after obtaining critical work permit. ","2020-05-18T23:59:35","","Completed","2020-04-25T23:59:35","No","No","No","Internal"]
[null,null,null,11617,null,"57_30/4/2020 2:50:17 AM","2020-04-18T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Emergency DG Radiator air inlet duct damper solenoid valve-air leak","Critical Equip.","Emgcy. Systems","Equipment Related","10.1","Medium","","","Solenoid valve of emcy DG overhauled and rectified the leak. System operation tried out-found working satisfactory","2020-05-18T23:59:35","","Completed","2020-04-18T23:59:35","No","No","No","Internal"]
[null,null,null,11618,null,"57_30/4/2020 2:45:27 AM","2020-04-18T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Emergency DG -Manual starting mode lamp not working","Elect. Mach. & Equip.","Emgcy. Systems","Equipment Related","10.1","Medium","","","Renewed the defective indication lamp","2020-05-03T23:59:35","","Completed","2020-04-18T23:59:35","No","No","No","Internal"]
[null,null,null,11619,null,"57_30/4/2020 2:59:44 AM","2020-04-18T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Garbage drums near incinerator loosely lashed","Miscellaneous","General Appearance","Equipment Related","10.1","Medium","","","Garbage drums wire lashing made tight","2020-04-28T23:59:35","","Completed","2020-04-23T23:59:35","No","No","No","Internal"]
[null,null,null,11620,null,"57_30/4/2020 3:03:25 AM","2020-04-18T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","O2 sensor near IG area showing O2 % 22","Miscellaneous","Safety / LSA / FFA","Equipment Related","10.1","Medium","","","O2 sensor calibrated. Now showing O2 -20.9 %","2020-05-03T23:59:35","","Completed","2020-05-18T23:59:35","No","No","No","Internal"]
[null,null,null,11621,null,"57_30/4/2020 3:12:40 AM","2020-04-18T23:59:35","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ME exhaust line dampers to be greased","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.1","Medium","","","All dampers greased.","2020-04-28T23:59:35","","Completed","2020-04-18T23:59:35","No","No","No","Internal"]
[null,null,null,11622,null,"57_23/4/2020 11:45:23 PM","2020-04-18T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Air cooler drain line modified","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.1","Medium","","","Drain connection put back to  normal.Hole made on the manhole cover welded with insert plate","2020-05-03T23:59:35","","Completed","2020-04-23T23:59:35","No","No","No","Internal"]
[null,null,null,11623,null,"57_30/4/2020 4:11:40 AM","2020-04-18T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","FWD/AFT HPU Cooler- Cavitation noise observed from","Deck - Machinery","Eng. / Strg. Comp.","Equipment Related","10.39","High","","","Routine practice for shutting cooler inlet valve already in practice.","2020-04-28T23:59:35","","Completed","2020-04-18T23:59:35","No","No","No","Internal"]
[null,null,null,11624,null,"57_30/4/2020 4:29:39 AM","2020-04-18T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Steam leak above ICO lube","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Steam line flange retightened- rectified steam leak","2020-04-28T23:59:35","","Completed","2020-04-18T23:59:35","No","No","No","Internal"]
[null,null,null,11625,null,"57_30/4/2020 4:41:38 AM","2020-04-18T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Cargo pumps and Ballast pumps- Bulkhead seal grease pot level below red mark","E/R - Aux. Mach.","Cargo / Ballast Systems","Equipment Related","10.1","Medium","","","Topped up grease to the red mark wherever level found below red mark.","2020-05-03T23:59:35","","Completed","2020-04-18T23:59:35","No","No","No","Internal"]
[null,null,null,11626,null,"57_30/4/2020 3:45:47 PM","2020-04-18T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Emergency fire pump room drain cock frozen","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.1","Medium","","","Drain cock overhauled - well lubricated and eased up- working satisfactorily.","2020-05-18T23:59:35","","Completed","2020-04-18T23:59:35","No","No","No","Internal"]
[null,null,null,11627,null,"57_23/4/2020 11:57:42 PM","2020-04-18T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","main switch board -220 V low insulation","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.24","Low","","","Traced out earth fault and rectified . Now reading b/w 10 and infinity","2020-05-03T23:59:35","","Completed","2020-04-25T23:59:35","No","No","No","Internal"]
[null,null,null,11628,null,"57_30/4/2020 4:17:33 AM","2020-04-18T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","DG 1,2,& 3 -Lagging missing from FO filter","E/R - Aux. Engine","Eng. / Strg. Comp.","Behaviour Based,Equipment Related","10.27","Medium","","","Laggings were removed for cleaning. Same put back in place. ","2020-04-28T23:59:35","","Completed","2020-04-18T23:59:35","No","No","No","Internal"]
[null,null,null,11629,null,"57_30/4/2020 4:04:53 AM","2020-04-18T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Hydrophore pumps-suction /discharge gauges showing 4.5 bar. NRV for hyd tank not holding","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.1","Medium","","","NRV renewed. Now both pump discharge pressure reads zero while st/by","2020-05-18T23:59:35","","Completed","2020-04-28T23:59:35","No","No","No","Internal"]
[null,null,null,11630,null,"57_30/4/2020 4:36:47 AM","2020-04-18T23:59:35","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Spare ME piston- Open both clamps and inspect fretting at clamping area","E/R - Main Engine","Eng. / Strg. Comp.","Knowledge Based","10.1","Medium","","","Opened both clamps and inspected clamping area- found in good condition - No signs of fretting.","2020-05-18T23:59:35","","Completed","2020-04-21T23:59:35","No","No","No","Internal"]
[null,null,null,12122,null,"57_4/6/2020 04:02:23","2020-04-22T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Fpk tk. gate v/v (450A) unable to be operated from main dk. (only manual op. for this v/v)","Hull & Tanks","Cargo / Ballast Systems","Equipment Related","8.11","Medium","","","On tank entry it was noted v/v stuck in position, v/v dismantled, found that gate flange was reversed (back to front) & open/shut hyd connections to hyd motor also reversed. v/v derusted, cleaned, painted & position of gate flange & hyd connections rectified. v/v now operating","2020-05-29T23:59:35","","Completed","2020-05-24T23:59:35","No","No","No","Internal"]
[null,null,null,12121,null,"57_2/6/2020 8:47:08 AM","2020-05-29T23:59:35","Defect","Ship Staff","Engineering Audit","ME Unit 2 liner and piston rings found scuffing heavily and worn out.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Unit 2 Cylinder lubrication increased. Pmax offset ME Unit 2 Piston and stuffing box renewed","2020-07-12T23:59:35","DSTA205039","Completed","2020-07-01T23:59:35","No","No","No","Internal","Spare liner will be supplied at Singapore on 2nd July."]
[null,null,null,12817,null,"57_24/6/2020 1:20:55 PM","2020-06-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Jacket cooling water found leaking into fresh water generator evaporator","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.1","Medium","","","FWG isolated and evaporator pressure tested. Found one tube leaking- same plugged using brass plug. Pressure tested again and found satisfactory.","2020-07-03T23:59:35","NA","Completed","2020-06-02T23:59:35","No","No","No","Internal"]
[null,null,null,15934,null,"57_20/12/2020 11:23:46 AM","2020-07-28T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","CW pressure gauge defective","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Pressure gauge renewed.","2020-08-05T23:59:35","","Completed","2020-08-01T23:59:35","No","No","No","Internal"]
[null,null,null,15935,null,"57_20/12/2020 11:26:19 AM","2020-07-28T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Central cooling FW cooler no. # 1 & 2 foundation has salt deposit. Identify source & rectify","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","SW inlet Filter gaskets renewed and leak rectified.","2020-08-05T23:59:35","","Completed","2020-08-03T23:59:35","No","No","No","Internal"]
[null,null,null,15936,null,"57_20/12/2020 11:29:59 AM","2020-07-28T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Cooler no. 1 & 2 back flush sheet not updated for last back flush","Documentation","Cert. & Docu.","Human Error","10.1","Medium","","","Back flush date updated.","2020-08-05T23:59:35","","Completed","2020-07-29T23:59:35","No","No","No","Internal"]
[null,null,null,15937,null,"57_20/12/2020 11:32:41 AM","2020-07-28T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Motor shaft seal oil glass empty","Deck - Machinery","Eng. / Strg. Comp.","Equipment Related","6.13","Low","","","Oil topped up.","2020-08-05T23:59:35","","Completed","2020-07-30T23:59:35","No","No","No","Internal"]
[null,null,null,15938,null,"57_20/12/2020 11:34:46 AM","2020-07-28T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Oil traces near drain valve. Identify source & rectify","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Drain valve tightened and leak rectified.","2020-08-12T23:59:35","","Completed","2020-08-02T23:59:35","No","No","No","Internal"]
[null,null,null,15939,null,"57_20/12/2020 11:37:14 AM","2020-07-28T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","LO tank normal level to mark","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.1","Medium","","","LO tank normal level marked.","2020-07-29T23:59:35","","Completed","2020-07-29T23:59:35","No","No","No","Internal"]
[null,null,null,15940,null,"57_21/12/2020 11:10:00 AM","2020-07-28T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","COT 3P IG line blank plate not at stowage location","Deck - Pipe / Fittings","Cargo / Ballast Systems","Human Error","8.23","Medium","","","3P IG line blank plates secured back at stowage location","2020-08-05T23:59:35","","Completed","2020-07-29T23:59:35","No","No","No","Internal"]
[null,null,null,15941,null,"57_21/12/2020 11:15:57 AM","2020-07-28T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Compass deck-Spot rust spots on hinges, stanchions etc to derust & paint","Accommodation","General Appearance","Equipment Related","11.8","Low","","","Spot derusting and painting maintenance completed.","2020-08-28T23:59:35","","Completed","2020-08-04T23:59:35","No","No","No","Internal"]
[null,null,null,13849,null,"57_11/8/2020 10:02:00 AM","2020-08-02T23:59:35","Defect","Ship Staff","Ship Staff Insp.","DG #2 centrifuge filter base flange cracked","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Received new LO centrifugal filter fitted in place with small modification in pipe line connection. Now in operation and working satisfactory.","2021-03-29T23:59:35","","Completed","2021-02-16T23:59:35","No","No","No","Internal","Spare is ready at Singapore. Will be supplied during bunker call."]
[null,null,null,13851,null,"57_11/8/2020 10:08:23 AM","2020-08-02T23:59:35","Defect","Ship Staff","Ship Staff Insp.","PA system amplifer defective","Miscellaneous","Safety / LSA / FFA","Equipment Related","11.16","Low","","","Defective transistors in the amplifiers on both the systems renewed. Need to check system performance","2020-08-29T23:59:35","","Completed","2020-08-10T23:59:35","No","No","No","Internal"]
[null,null,null,13852,null,"57_19/8/2020 3:34:59 PM","2020-08-05T23:59:35","Defect","Ship Staff","Ship Staff Insp.","MF /HF Antenna was damaged during rough weather","Navigation - GMDSS & Communication","Communication","External Factors","4.23","High","","","Requisition DSTA205057 was supplied and defective MF/HF Antenna was renewed.","2020-08-13T23:59:35","DSTA205057","Completed","2020-08-11T23:59:35","No","No","No","Internal"]
[null,null,null,13853,null,"57_19/8/2020 3:41:46 PM","2020-08-05T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Stbd Gangway :One shifting wire broken ,same to be renewed.","Miscellaneous","Safety / LSA / FFA","Equipment Related","5.47","Medium","","","Damaged shifting wire renewed with spare.","2020-08-13T23:59:35","NA","Completed","2020-08-08T23:59:35","No","No","No","Internal"]
[null,null,null,13855,null,"57_11/8/2020 10:10:31 AM","2020-08-06T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Hotwell gauge glass leaking.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Gaugle glass renewed leak arrested.","2020-08-13T23:59:35","","Completed","2020-08-08T23:59:35","No","No","No","Internal"]
[null,null,null,13850,null,"57_19/8/2020 3:59:31 PM","2020-08-08T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Gangway falls and shifting wires are in service since vessels delivery ( Installed On 27th April 2018), same to be renewed every 24M as per GSM SAFETY CIRCULAR/S-001-2019 - POINT NO 6","Miscellaneous","ISM Related","Equipment Related","5.47","Medium","","","Gangway Falls Renewed On 24th Oct 2020.","2020-12-29T23:59:35","DSTA-200175: Received ","Completed","2020-10-22T23:59:35","No","No","No","Internal"]
[null,null,null,13848,null,"57_19/8/2020 5:12:08 PM","2020-08-09T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Echo Sounder Printer Thermal head is malfunctioning & requires replacement, as the data print is unreadabale.","Navigation - Echo Sounder / Speed Log","Navigation","Equipment Related","4.19","Low","","","Spares received and Echo Sounder Thermal Printer Head renewed.","2020-12-29T23:59:35","DSTA-205063-Received","Completed","2020-10-12T23:59:35","No","No","No","Internal"]
[null,null,null,14358,null,"57_14/9/2020 4:18:38 PM","2020-08-12T23:59:35","Observation","Ship Staff","Ship Staff Insp.","DG #1 and #3 T/C exh gas inlet temp gauge not working","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.33","High","","","DSTA200070 raised, cancelled from office. Requesition raised again DSTA210034, SPARES RECEIVED AT SINGAPORE, REPLACEMENT OF SENSOR IS GOING ON. COMPLETED.","2021-01-29T23:59:35","DSTA210034","Completed","2021-01-13T23:59:35","No","No","No","Internal","Will be supplied at Singapore during bunker call."]
[null,null,null,13854,null,"57_15/8/2020 2:06:29 PM","2020-08-13T23:59:35","Critical Equipment","Ship Staff","Ship Staff Insp.","Stbd lifeboat engine not starting","LSA / FFA","Safety / LSA / FFA","Equipment Related","10.6","Very High","","","Starting motor overhauled. engine tried out on both batteries, working satisfactory.","2020-08-13T23:59:35","","Completed","2020-08-13T23:59:35","No","No","No","Internal"]
[null,null,null,14363,null,"57_8/9/2020 6:38:38 AM","2020-08-18T23:59:35","Defect","Ship Staff","Ship Staff Insp.","DG #2 unit 1 fuel valve pocket sleeve o-ring damaged resulting in water leak","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Unit 1 fuel valve sleeve O-rings renewed with new spare","2020-08-29T23:59:35","","Completed","2020-08-20T23:59:35","No","No","No","Internal"]
[null,null,null,14357,null,"57_16/9/2020 11:43:27 PM","2020-08-21T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Pilot ladder onboard  do not comply with GSM  Safety Flash 20120420","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.47","Medium","","","1 NEW PILOT LADDER SUPPIED -STBD SIDE PILOT LADDER RENEWED.","2021-02-26T23:59:35","DSTA210007","Completed","2021-01-18T23:59:35","No","No","No","Internal","Will be supplied at Singapore."]
[null,null,null,14364,null,"57_8/9/2020 6:43:20 AM","2020-08-22T23:59:35","Defect","Ship Staff","Ship Staff Insp.","# steam leaks in E/rm to be rectified","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Steam leaks rectified as the vessel was in port","2020-08-29T23:59:35","","Completed","2020-08-29T23:59:35","No","No","No","Internal"]
[null,null,null,14359,null,"57_16/9/2020 11:54:12 PM","2020-08-28T23:59:35","Critical Equipment,Observation","Ship Staff","Ship Staff Insp.","One tank overfill alarm light (Stbd side midhship / aft light) was not operational.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.14","Very High","","","Tank Overfill Alarm Light Renewed.","2020-12-29T23:59:35","DSTA200177:Requisition raised for spare horn and light.","Completed","2020-08-29T23:59:35","No","No","No","Internal"]
[null,null,null,14365,null,"57_8/9/2020 6:35:48 AM","2020-08-31T23:59:35","Defect","Ship Staff","Engineering Audit","ME Unit 7 FIVA accumulator found with 26 bars pressure","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Accumulator renewed with new spare","2020-09-03T23:59:35","","Completed","2020-09-01T23:59:35","No","No","No","Internal"]
[null,null,null,14360,null,"57_16/9/2020 11:47:46 PM","2020-09-07T23:59:35","Defect,Observation","Ship Staff","Ship Staff Insp.","The fabric material condition of the stretcher in Pumproom has deteriorated. Additionally, the straps were observed to be broken.","Miscellaneous","Safety / LSA / FFA","Equipment Related","5.2","Very High","","","New stretcher received and put  in service","2020-12-15T23:59:35","DSTA200182-Received","Completed","2020-10-12T23:59:35","No","No","No","Internal"]
[null,null,null,14361,null,"57_17/9/2020 12:00:49 AM","2020-09-08T23:59:35","Non Conformity,Observation","Ship Staff","Ship Staff Insp.","Working life vests not SOLAS Compliant.","LSA / FFA","Safety / LSA / FFA","Equipment Related,Knowledge Based","5.32","High","","","Requisition Received- New SOLAS Compliant Work Vest Used .","2020-12-08T23:59:35","DSTA-200178 -Received","Completed","2020-10-12T23:59:35","No","No","No","Internal"]
[null,null,null,14362,null,"57_17/9/2020 12:48:49 AM","2020-09-13T23:59:35","Defect,Observation","Ship Staff","Ship Staff Insp.","CCR remote ballast level readings are erratic , system requires to be rebooted occassionally .","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.18","High","","","one HPI-100 PCB renewed for bunker tanks, another PCB also renewed. Working satisfactory. Job order no: V-DSTA020978/21","2021-02-26T23:59:35","","Completed","2021-01-27T23:59:35","No","No","No","Internal","Spare will be supplied while passing Singapore around 25th Dec."]
[null,null,null,15295,null,"57_25/11/2020 5:12:34 PM","2020-09-15T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Sea water leakage from main sea water pump #2","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Mechanical seal renewed. RO raised for spare seal.","2020-09-18T23:59:35","DSTA200204","Completed","2020-09-16T23:59:35","No","No","No","Internal"]
[null,null,null,15296,null,"57_25/11/2020 5:18:51 PM","2020-09-18T23:59:35","Critical Equipment","Ship Staff","Ship Staff Insp.","High expension foam system proportioner valve diaphgram damage","LSA / FFA","Safety / LSA / FFA","Industry Issue","5.35","Medium","","","Proportioner valve diaphgram renewed.","2020-09-28T23:59:35","","Completed","2020-09-21T23:59:35","No","No","No","Internal"]
[null,null,null,15297,null,"57_25/11/2020 5:22:22 PM","2020-09-20T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","ME unit no 2 exhaust valve not operating","E/R - Main Engine","Eng. / Strg. Comp.","Industry Issue","10.1","Medium","","","Unit no 2 exh valve,fiva valve,MPC,exhaust valve actuator, LO HP pipe renewed during trobleshooting. LO HP pipe found damaged.","2020-09-20T23:59:35","","Completed","2020-09-20T23:59:35","No","No","No","Internal"]
[null,null,null,15298,null,"57_25/11/2020 5:31:00 PM","2020-09-22T23:59:35","Defect","Ship Staff","Ship Staff Insp.","ME unit no & fuel oil leak off alarm getting activated","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.1","Medium","","","Distributer to fuel valve aft and middle pipe renewed. fwd pipe replaced with overhauled one. booster to distribution block pipe lapping carried out and leak rectified.","2020-09-23T23:59:35","","Completed","2020-09-22T23:59:35","No","No","No","Internal"]
[null,null,null,15299,null,"57_25/11/2020 5:33:52 PM","2020-10-02T23:59:35","Defect","Ship Staff","Ship Staff Insp.","ME unit no 3 FO HP pipe leaking from outer pipe (booster to distribution block)","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.1","Medium","","","Surface lapping carried out and pipe replaced with overhauled pipe.","2020-10-03T23:59:35","","Completed","2020-10-02T23:59:35","No","No","No","Internal"]
[null,null,null,15304,null,"57_25/11/2020 5:36:55 PM","2020-10-12T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Main engine Aux Blower #2 was not operating due to main contactor holding coil failure.","E/R - Main Engine","Eng. / Strg. Comp.","Industry Issue","10.1","Medium","","","Main contactor renewed. Requesition raised for spare contactor.","2020-10-12T23:59:35","DSTA200213","Completed","2020-10-12T23:59:35","No","No","No","Internal"]
[null,null,null,15300,null,"57_25/11/2020 5:43:28 PM","2020-10-13T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Various steam leaks- Above ico lube unit, Above ME SCR unit and 6K dump valve flanges","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Industry Issue","10.29","Medium","","","Gaskets renewed and leak rectified.","2020-10-18T23:59:35","","Completed","2020-10-14T23:59:35","No","No","No","Internal"]
[null,null,null,15301,null,"57_25/11/2020 5:46:53 PM","2020-10-17T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Aft hydraulics LO leak from HP pipe flange inside steering gear room","Deck - Mooring Machinery","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","O ring renewed and leak rectified.","2020-10-18T23:59:35","","Completed","2020-10-18T23:59:35","No","No","No","Internal"]
[null,null,null,15302,null,"57_25/11/2020 8:59:42 PM","2020-10-24T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Main engine unit no 6 FO HP pipe leak","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.19","Very High","","","FO pipe booster pump to distributor block removed. surface lapping carried out and leak rectified.","2020-10-25T23:59:35","","Completed","2020-10-24T23:59:35","No","No","No","Internal"]
[null,null,null,15303,null,"57_25/11/2020 9:08:05 PM","2020-10-25T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Main engine unit #5 exhaust valve stroke was less compaired to other units","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.21","Medium","","","Exhaust valve spring air safety valve replaced with overhauled one.","2020-10-28T23:59:35","","Completed","2020-10-25T23:59:35","No","No","No","Internal"]
[null,null,null,15305,null,"57_25/11/2020 9:10:19 PM","2020-10-25T23:59:35","Defect","Ship Staff","Ship Staff Insp.","AE 3 fresh water attach pump seal leakage","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Seal renewed","2020-10-28T23:59:35","","Completed","2020-10-27T23:59:35","No","No","No","Internal"]
[null,null,null,15306,null,"57_25/11/2020 9:14:20 PM","2020-10-27T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Valve remote control system hydraulic leak from valve control block flowmeter CL151","Deck - Machinery","Eng. / Strg. Comp.","Equipment Related","10.1","Medium","","","O ring renewed and leak rectified. Requestion raised for sapare o ring.","2020-10-31T23:59:35","DSTA200220","Completed","2020-10-29T23:59:35","No","No","No","Internal"]
[null,null,null,15289,null,"57_26/11/2020 7:03:32 PM","2020-11-11T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Fwd Fire Wire Winch- Reduction Gear Defective","Deck - Mooring Machinery","Mooring","Equipment Related","9.14","Medium","","","Requisition DSTA200218 received at singapore on 14th Jan 2021.Reduction gear box overhauled and defective parts replaced. Fwd fire wire reel now in operatitional rediness.","2021-02-11T23:59:35","DSTA200218","Completed","2021-01-16T23:59:35","No","No","No","Internal","PO issued. Awaiting spare readiness."]
[null,null,null,15294,null,"57_26/11/2020 6:53:50 PM","2020-11-11T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Pumproom & Engine room TRO- N (Neutralising agent tank) Level sensor defective.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","6.21","High","","","Both pump room and engine room level sensors replaced with spare new ones. Now both the level sensors are operational and showing the correct reading. Job order no: V-DSTA021223/21","2021-02-11T23:59:35","","Completed","2021-02-03T23:59:35","No","No","No","Internal","PO issued. Awaiting spare readiness."]
[null,null,null,15292,null,"57_26/11/2020 7:08:47 PM","2020-11-17T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Mooring winch brake band regulating screws required to be freed up .","Deck - Mooring Machinery","Mooring","Equipment Related","9.14","Medium","",""," Mooring winch brake band regulating screws have been  lubricated and freed.","2021-02-17T23:59:35","","Completed","2020-11-27T23:59:35","No","No","No","Internal","Noted, update progress in weekly deck maintenance report."]
[null,null,null,15290,null,"57_26/11/2020 7:24:05 PM","2020-11-18T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Two fire hoses observed to be leaking during pressure test.","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.35","Medium","","","Fire hose renewed.Defective fire hoses repaired and made good.","2021-02-18T23:59:35","","Completed","2021-11-20T23:59:35","No","No","No","Internal","Raise requisition after 31st Dec.  This can be closed, since it is not a defect. Spare rope tails will be supplied before expiry."]
[null,null,null,15291,null,"57_26/11/2020 7:13:54 PM","2020-11-18T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Fixed Gas Detection System 30M Shore Service Not Carried Out.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","5.21","Medium","","","New RO DSTA210011 raised for 30M Shore Service of Fixed Gas Detection System  In Jan 2021. Planned to be conducted at vessels next call Singapore around 12th Jan 2021. SHORE TECHNICIAN ATTANDED VESSEL AT SINGAPORE ON 14TH JAN 2021 AND SHORE SERVICEING CARRIED OUT. ","2021-02-18T23:59:35","DSTA210011 & DSTA210012","Completed","2021-01-12T23:59:35","No","No","No","Internal","Awaiting quotation for sensor. For 30M service, raise requisition again after 31st Dec. Will arrange in Jan 2021, when vessel calls for bunkers."]
[null,null,null,15293,null,"57_26/11/2020 7:31:00 PM","2020-11-22T23:59:35","Observation","Ship Staff","Ship Staff Insp.","4S COT VAPOUR PRESSURE READING IN CCR IS ERRATIC.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.19","High","","","VAPOR PRESSURE SENSOR DISCONNECTED AND RESTARTED ,DEFECT OBSERVED TO BE RECTIFED.","2021-02-22T23:59:35","","Completed","2021-11-24T23:59:35","No","No","No","Internal","Raise requisition after 31st Dec."]
[null,null,null,15872,null,"57_2/12/2020 2:08:46 PM","2020-11-23T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Fresh water genrator distillate pump leakage from seal","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Mechanical seal renewed and requesition raised for spare seal.","2020-11-25T23:59:35","DSTA200223","Completed","2020-11-24T23:59:35","No","No","No","Internal"]
[null,null,null,15867,null,"57_2/12/2020 2:19:50 PM","2020-11-24T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Fresh water genrator ejector pump was not staring,found pump start delay time relay faulty","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.37","Medium","","","pump start delay time relay interchanged from winding heater delay time relay. requesition raised for relay to renew winding heater delay time relay. WORK COMPLETED, ON FWG EJECTOR PUMP AND IS WORKING SATISFACTORY, REQUISITION DSTA200223 PENDING, CLOSING DEFECT. ","2021-01-29T23:59:35","DSTA200223","Completed","2021-01-10T23:59:35","No","No","No","Internal"]
[null,null,null,15873,null,"57_14/12/2020 6:39:40 AM","2020-12-04T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Stripping pump steam return line leakage near LO cooler and above soot tank.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.1","Medium","","","Both flanges gaskets renewed, leak rectified.","2020-12-08T23:59:35","","Completed","2020-12-05T23:59:35","No","No","No","Internal"]
[null,null,null,15868,null,"57_15/12/2020 8:55:32 AM","2020-12-06T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Personal Multi gas detector MSA ALTAIR 4XR- Serial Number 06020321 is observed to be showing “Sensor Error” during its startup sequence .","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","5.23","Very High","","","Personal Multi gas detector MSA ALTAIR 4XR- Serial Number 06020321 has been replaced under IM&M Warrenty on 17th Dec 2020-Singapore Transit","2021-03-06T23:59:35","","Completed","2020-12-15T23:59:35","No","No","No","Internal","Spare supplied while passing Singapore. Close defect."]
[null,null,null,15869,null,"57_14/12/2020 22:45:31","2020-12-10T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Fixed Gas Detection System GS5000: IG Blower area Oxygen sensor  is defective.Oxygen reading shows 25% Vol.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","5.21","Medium","","","Sensor interchanged with other area, found sensor defective.Requisition DSTA210006 raised in Jan 2021 for spare sensor. SPARES RECEIVED AT SINGAPORE, BUT BEFORE REPLACEMENT OF PARTS, VESSEL CHECKED SENSORS AGAIN AND NOW O2 READING IS SHOWING CORRECT.  RECEIVED SPARES KEPT FOR FUTURE USE, JOB COMPLETED","2021-03-10T23:59:35","DSTA210006","Completed","2021-01-13T23:59:35","No","No","No","Internal","Raise requisition ASAP to supply at Singapore bunker call."]
[null,null,null,15874,null,"57_14/12/2020 6:43:53 AM","2020-12-12T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Sludge pump priming fresh water supply valve spindle sheared off.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Valve renewed.","2020-12-12T23:59:35","","Completed","2020-12-12T23:59:35","No","No","No","Internal"]
[null,null,null,15870,null,"57_14/12/2020 23:05:31","2020-12-13T23:59:35","Observation","Ship Staff","Ship Staff Insp.","IG line vent valve before deck seal observed to have a pneumatic leak.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.22","Very High","","","Pneumatic actuator overhauled and O Ring renewed, IG line vent valve pneumatic leak rectified.","2021-03-13T23:59:35","","Completed","2020-12-15T23:59:35","No","No","No","Internal","Raise this in email when you send UTI for calibration. Since this is not a defect,  not worth keeping in DDRL. Close this observation in DDRL."]
[null,null,null,15871,null,"57_15/12/2020 9:24:21 AM","2020-12-13T23:59:35","Defect","Ship Staff","Ship Staff Insp.","During inspection of ballast tank vent heads it was observed that the forepeak water ballast tank vent head, inner seal ring was found missing .The float is damaged and is misaligned.","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","Equipment Related","8.1","Very High","","","Requisition DSTA200196 received at Singapore on 14th Jan 21. Fpk WBT vent overhauled ,Float & seal ring renewed. Fpk vent in operational condition.","2021-03-13T23:59:35","DSTA200196","Completed","2021-01-20T23:59:35","No","No","No","Internal","Will be supplied at Singapore bunker call."]
[null,null,null,15942,null,"57_20/12/2020 11:49:57 AM","2020-12-16T23:59:35","Defect","Ship Staff","Ship Staff Insp.","ALL 3 COPT steam line supports found loose.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.1","Medium","","","Steam line supports alignened and tightened.","2020-12-18T23:59:35","","Completed","2020-12-17T23:59:35","No","No","No","Internal"]
[null,null,null,15933,null,"57_20/12/2020 12:05:34 PM","2020-12-18T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Sea water seepage from LT cooler vent valve connection.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Vent valve connection renewed and leak rectified.","2020-12-29T23:59:35","","Completed","2020-12-26T23:59:35","No","No","No","Internal","Plan to rectify defect at Port stay in China."]
[null,null,null,16698,null,"57_5/1/2021 7:48:27 AM","2020-12-21T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Aux Boiler No 1 water level gauge glass leakage","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.1","Medium","","","Gauge glass gaskets renewed and leak rectified.","2020-12-22T23:59:35","","Completed","2020-12-21T23:59:35","No","No","No","Internal"]
[null,null,null,16696,null,"57_5/1/2021 7:36:28 AM","2020-12-24T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Low sea chest MGPS module TC2 defective","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.33","High","","","Module to renew. Requesition raised for spare, SPARES RECEIVED MGPS MODULE CARD REPLACED, DEFECT RECTIFIED, MGPS SYSTEM BACK TO NORMAL. ","2021-03-29T23:59:35","DSTA200251","Completed","2021-01-13T23:59:35","No","No","No","Internal","Will be supplied at Singapore on 13th Jan."]
[null,null,null,16697,null,"57_5/1/2021 7:40:53 AM","2020-12-26T23:59:35","Defect","Ship Staff","Ship Staff Insp.","PA System amplifier unit defective.","Elect. Mach. & Equip.","Communication","Equipment Related","10.33","High","","","Trobuleshooting in progress. SPARES RECEIVED AT SINGAPORE ON 14TH JAN 2021, VESSEL CHANGED ALL ELECTRICAL CARDS ON SYSTEM, PA SYSTEM BACK IN OPERATION, JOB COMPLED","2021-03-29T23:59:35","","Completed","2021-01-13T23:59:35","No","No","No","Internal","Locate equipment which is giving short circuit."]
[null,null,null,17569,null,"57_13/1/2021 2:12:17 AM","2021-01-06T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","MCSW pump No 1 not operational due to falty VFD","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.37","Medium","","","VFD internal component got damaged. Requesition raised for same. DSTA210043, Need shore assitance for fault rectification, Need to land VFD at Singapore and receive it back after repairs. Management has decided to give new VFD, And for emerengy purposes one DOL is given at Singapore, DOL mounting stand  fabrication  is going on and job will get complete before month end. Once DOL in place we can close this job. DOL STARTER PANEL INSTALLED. PUMP TRIED OUT. ALL SATISFACTORY< PUMP NO-1 IS BACK IN USE.","2021-05-29T23:59:35","DSTA210043,","Completed","2021-04-27T23:59:35","No","No","No","Internal","Order placed for spare VFD. Also arrange one DOL starter for the pump, to operate till receipt of VFD."]
[null,null,null,17570,null,"57_13/1/2021 3:46:16 AM","2021-01-08T23:59:35","Defect","Ship Staff","Ship Staff Insp.","ME SCR blower sealing air line pressure regulator defective","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.1","Medium","","","Pressure regulator replaced with spare new one. Job order no: V-DSTA020948/21","2021-02-26T23:59:35","","Completed","2021-01-25T23:59:35","No","No","No","Internal"]
[null,null,null,2589,null,"57_20/10/2019 4:54:32 PM","2021-01-10T23:59:35","Defect","Ship Staff","Ship Staff Insp.","BWTS unit, inside filter unit many cleaning nozzles found in siezed and worn out condition.","Deck - Machinery","Cargo / Ballast Systems","Equipment Related","6.21","High","","","Spares received at Singapore on 5th march-2020, to be attended, vessel in progress of rectifing faults on No-2 Filter, Two new filters installed inside No-2 filter casing.VESSEL OPENED LOOP TWO FILTER AND CHANGED TWO FILTERS CARTRIDGE, ALL SEALING ARRANGEMENT FOR BACK FLUSH SYSTEM CHANGED , FILTER TRIED OUT ALL SATISFACTORY. VESSEL IS RAISING REQUISITION FOR SPARE NOZZLES AND SPARES FOR FILTERS","2021-05-29T23:59:35","","Completed","2021-04-23T23:59:35","No","No","No","Internal","Spare is freighted to Singapore. Will be supplied during bunker call."]
[null,null,null,16695,null,"57_5/1/2021 7:32:53 AM","2021-01-15T23:59:35","Defect","Ship Staff","Ship Staff Insp.","FWD ICCP not working","Hull & Tanks","Eng. / Strg. Comp.","Equipment Related","10.37","Medium","","","Job carried out by service engineer. faulty thyristor renewed. System is operational and back to normal. Job order no: V-DSTA022074/21","2021-03-29T23:59:35","","Completed","2021-03-23T23:59:35","No","No","No","Internal","Service engineer will be arranged at Singapore."]
[null,null,null,17884,null,"57_10/2/2021 4:08:13 PM","2021-02-03T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Central FW cooler AFT #2 SW outlet pipe leakage at the instrument flange.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Removed the pipe and instrument flange. All the surfaces cleaned. New gasket joints put in place. The cooler pressure tested and observed no leakage from the flange. The flange observed to be erroded from inner side. Same cleaned and put back. RO raised for the same for future use. Job order : V-DSTA021222/21, Vessel received two flanges under requisition DSTA210045, And also vessel has rectified leak. Spare flanges will be use in future for same leak - At present we can decide job completed. ","2021-04-28T23:59:35","DSTA210045","Completed","2021-04-08T23:59:35","No","No","No","Internal","Spare already supplied to vessel on 1st April."]
[null,null,null,18103,null,"57_28/2/2021 12:31:05 PM","2021-02-24T23:59:35","Observation","Ship Staff","Ship Staff Insp.","HFO purifier supply pump #2 seal leakage to rectify and motor overhaul.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","The pump dismantled and inspected for any sign of seal damage, foundmechanical seal in damaged condition, same replaced with new one.\n\nThe pump bearing and rotors inspected, found in good condition.\n\nThe motor dismantled by ETO, both the bearings renewed. Stator and rotor observed to be in good condition.\n\nPump and motor boxed back with new coupling pad as it was not in place and found in broken small pieces. Job order no: V-DSTA021457/21\n\nNew teflon coupling pad made and fitted in place.\n\nThe pump tried out found working satisfactory. No abnormal noise, vibration and no seal leakage observed. Pump suction pr: 0.1 bar Discharge pr: 1.20 bar","2021-02-26T23:59:35","","Completed","2021-02-24T23:59:35","No","No","No","Internal"]
[null,null,null,18742,null,"57_14/4/2021 2:35:55 PM","2021-03-23T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ODME pressure switch diaphragm damaged and leakage occured.","Critical Equip.","MARPOL Related","Equipment Related","6.13","Low","","","Pressure switch to be renewed. Though ODME is working normally.","2021-07-23T23:59:35","DSTA210086","Completed","2021-07-12T23:59:35","No","No","No","Internal","Spare will be supplied next call Singapore."]
[null,null,null,18746,null,"57_14/4/2021 2:38:18 PM","2021-03-23T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Cooling fan for ER fan control panel not operational.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Cooling fan overhauled and now working satisfactory. ","2021-05-23T23:59:35","","Completed","2021-03-24T23:59:35","No","No","No","Internal"]
[null,null,null,18747,null,"57_14/4/2021 2:41:13 PM","2021-03-23T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Sewage treatment plant sludge recirculation not operational.","Documentation,E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Sewage treatment plant cleaned, Circulation pipe cleared, Operation checked all satisfactory","2021-04-03T23:59:35","","Completed","2021-03-30T23:59:35","No","No","No","Internal"]
[null,null,null,18748,null,"57_14/4/2021 2:43:29 PM","2021-03-23T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ER Bell book entries not complying with guidelines. Entries to be made as per guidelines given in the first page.","Documentation","Eng. / Strg. Comp.","Inappropriate Procedure","10.5","Low","","","All entries checked, and corrected, All engineers were shown what all entries are required and wording of entries explained","2021-04-03T23:59:35","","Completed","2021-03-30T23:59:35","No","No","No","Internal"]
[null,null,null,18475,null,"57_31/3/2021 2:30:19 PM","2021-03-28T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Incinerator waste oil settling tank No-1 and No-2 steam extraction fan seals are leaking","E/R - Aux. Mach.","MARPOL Related","Equipment Related","10.32","Very High","","","Need to replace seals and bearings on steam extraction fans (vessel does not have spare seals for extraction fan, Requisition DSTA210083 raised)","2021-07-28T23:59:35","DSTA210083","Completed","2021-07-13T23:59:35","No","No","No","Internal","Noted."]
[null,null,null,18476,null,"57_31/3/2021 2:36:10 PM","2021-03-28T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Fresh Water generator salinometer defective, not showing any PPM reading.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.1","Medium","","","Vessel need to replace defective salinometer probe and meter to resolve fault. Vessel does not have spare salinometer on board requisition DSTA210081 raised for same. Vesel found one spare salinometer on board wich was replaced in place of defective salinometer. DSTA210081 has been approved by management will come on board in future. At present job completed. ","2021-06-28T23:59:35","DSTA210081","Completed","2021-04-07T23:59:35","No","No","No","Internal","One spare sensor was supplied to vessel in Jan 2020. Please check."]
[null,null,null,18743,null,"57_12/4/2021 00:40:44","2021-04-05T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Spot rust on port pump room exhaust vent.","Miscellaneous","General Appearance","Equipment Related","11.3","Medium","","","Derusting and painting carried out","2021-05-20T23:59:35","","Completed","2021-05-19T23:59:35","No","No","No","Internal","Update progress on weekly deck maintenance report."]
[null,null,null,18744,null,"57_12/4/2021 00:45:26","2021-04-05T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Spot rust on Port and Stbd cargo manifold tray","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.3","Medium","","","Derusting and painting carried out, markings done.","2021-05-20T23:59:35","","Completed","2021-05-15T23:59:35","No","No","No","Internal","Update progress on weekly deck maintenance report."]
[null,null,null,18745,null,"57_12/4/2021 00:48:18","2021-04-05T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Spot rust on pipe supports on main deck.","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.7","High","","","Maintenance works completed from 5X COT to Accomodation front","2021-07-05T23:59:35","","Completed","2021-06-22T23:59:35","No","No","No","Internal","Update progress on weekly deck maintenance report."]
[null,null,null,19647,null,"57_19/5/2021 11:05:18 AM","2021-04-11T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Spacer to be added to Aux. Engine LO thermostat as per Yanmar DG service letter","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Requisition raised. Awaiting for spares.","2021-07-29T23:59:35","DSTA210089","Completed","2021-07-12T23:59:35","No","No","No","Internal","Will be supplied next Singapore call."]
[null,null,null,19649,null,"57_28/5/2021 9:13:07 PM","2021-05-04T23:59:35","Observation","Ship Staff","Ship Staff Insp.","The aux boiler no 2 FD fan outlet canvas bellow observed damaged at two places causing air ingress.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","The damaged canvas bellow replaced with spare new one. FD fan tried out, found working satisfactory.","2021-05-29T23:59:35","","Completed","2021-05-29T23:59:35","No","No","No","Internal"]
[null,null,null,19513,null,"57_15/5/2021 8:50:03 AM","2021-05-07T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Sludge pump not able to make delivery up to incinerator waste oil tanks, ","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.31","Very High","","","Overhaul Pump is needed, Pump overhauled on 9th May , Stator of pump found completely wasted. new stator mounted on pump, Pump tried out , all satisfactory. ","2021-05-09T23:59:35","","Completed","2021-05-07T23:59:35","No","No","No","Internal"]
[null,null,null,19512,null,"57_15/5/2021 9:02:35 AM","2021-05-12T23:59:35","Defect","Ship Staff","Ship Staff Insp.","BWTS system, Ballast Loop two, TRO unit sample drain pump is defective (Not pumping)","Deck - Machinery,Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.14","Very High","","","Drain pump dismantled and overhalued. The function checked during BWTS Loop 2 trial, found working satisfactory.","2021-05-18T23:59:35","","Completed","2021-05-12T23:59:35","No","No","No","Internal","Overhaul pump and rectify defect."]
[null,null,null,19650,null,"57_1/6/2021 8:01:06 PM","2021-05-28T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Oxygen Sensor of SALWICO Gas detecting system near IG fan- IG scrubber platform defective. Showing O2%-25% by volume. ","Elect. Mach. & Equip.","Safety / LSA / FFA","Equipment Related","10.37","Medium","","","O2 Sensor replaced with new one.  ","2021-06-01T23:59:35","","Completed","2021-05-29T23:59:35","No","No","No","Internal"]
[null,null,null,19781,null,"57_14/6/2021 6:41:26 PM","2021-05-30T23:59:35","Defect","Ship Staff","Ship Staff Insp.","HFO Purifier Feed pump number 2 observed to be running with abnormal noise.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","The pump dismantled, found rotor bearing damaged, same renewed. All the parts cleaned and inspected, all found in order.","2021-06-28T23:59:35","","Completed","2021-06-02T23:59:35","No","No","No","Internal"]
[null,null,null,19782,null,"57_14/6/2021 6:55:46 PM","2021-05-30T23:59:35","Defect","Ship Staff","Ship Staff Insp.","AE2 turbocharger exhaust gas inlet temp sensor malfunctioning. ","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Removed and calibrated, found not functional. Replaced with new one, showing correct reading.","2021-06-05T23:59:35","","Completed","2021-05-31T23:59:35","No","No","No","Internal"]
[null,null,null,19783,null,"57_14/6/2021 6:22:44 PM","2021-05-30T23:59:35","Observation","Ship Staff","Ship Staff Insp.","ME unit no 3 FO booster unit HP pipe obersved leaking from distribution unit.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.3","Medium","","","Both the HP pipe replaced with spare overhauled one. The seating faces cleaned of accumulations. No leakage present after engine running.","2021-06-02T23:59:35","","Completed","2021-05-31T23:59:35","No","No","No","Internal"]
[null,null,null,19981,null,"57_29/6/2021 13:10:35","2021-06-26T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Spot rust on pipe support on main deck","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.7","High","","","Maintenance done on pipe supports.Derusting and painting carried out.","2021-11-28T23:59:35","","Completed","2021-10-28T23:59:35","No","No","No","Internal","Report progress in weekly deck maintenance report."]
[null,null,null,19982,null,"57_30/6/2021 12:20:41 PM","2021-06-27T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Sewage Treatment Plant,Vacuumarator pump#1 leaking from front cover due to minor crack was developed near the bottom cover tightening bolt.","E/R - Aux. Mach.","MARPOL Related","Equipment Related,External Factors,Inappropriate Procedure","10.32","Very High","","","cold work applied and leak is rectified.","2021-09-28T23:59:35","DSTA210141","Completed","2021-09-06T23:59:35","No","No","No","Internal","PO issued. Waiting spare readiness."]
[null,null,null,20729,null,"57_29/8/2021 5:31:03 AM","2021-06-30T23:59:35","Defect,Observation","Ship Staff","Ship Staff Insp.","HFO PFR FEED PUMP #2 COUPLING MODIFIED FOR TEFLON MATERIAL","E/R - Pumps","Eng. / Strg. Comp.","Behaviour Based,Equipment Related,External Factors,Inappropriate Procedure","10.32","Very High","","","OEM SPARES TO BE INSTALLED.","2021-09-28T23:59:35","DSTA210145","Completed","2021-09-02T23:59:35","No","No","No","Internal","Please send details in email"]
[null,null,null,20069,null,"57_15/7/2021 8:16:28 AM","2021-07-03T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Few P/V valves for COTs found to be leaking.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.31","High","","","Lapping of required valves completed, no leakages observed. all working in good condition","2021-10-02T23:59:35","","Completed","2021-08-14T23:59:35","No","No","No","Internal","Noted. Update progress in weekly deck maintenance report."]
[null,null,null,20070,null,"57_15/7/2021 8:18:54 AM","2021-07-03T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Poop deck area upgradation, including derusting of Mooring winches required","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.7","High","","","Derusting and painting completed.","2021-10-02T23:59:35","","Completed","2021-08-16T23:59:35","No","No","No","Internal","Noted progress."]
[null,null,null,20737,null,"57_17/8/2021 7:29:02 PM","2021-07-08T23:59:35","Critical Equipment,Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ER foam system SSV & MV1 not in auto position.","Critical Equip.","Safety / LSA / FFA","Behaviour Based,Equipment Related,Human Error,Inappropriate Procedure,Knowledge Based","5.38","High","","","valves are in auto position.","2021-07-18T23:59:35","","Completed","2021-07-10T23:59:35","No","No","No","Internal"]
[null,null,null,20738,null,"57_17/8/2021 7:24:26 PM","2021-07-08T23:59:35","Defect,Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Galley/laundry 220V insulation at 3 mega ohm.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related,External Factors,Human Error,Inappropriate Procedure","10.32","Very High","","","Low Insulation alarm to be identified.","2021-09-08T23:59:35","","Completed","2021-07-11T23:59:35","No","No","No","Internal"]
[null,null,null,20739,null,"57_17/8/2021 7:27:13 PM","2021-07-08T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","PA system fault detector block defective and some of the cabins speaker is not working","Elect. Mach. & Equip.","Safety / LSA / FFA","Equipment Related,External Factors,Human Error,Inappropriate Procedure","10.33","High","","","Faul detector block connected to the power supply and no alarm are observed on unit display.","2021-09-08T23:59:35","","Completed","2021-08-23T23:59:35","No","No","No","Internal"]
[null,null,null,20740,null,"57_25/8/2021 9:25:38 PM","2021-07-08T23:59:35","Defect,Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","PA System Fault Detector is defective and some of the cabins speaker not in working condition\n\n","Elect. Mach. & Equip.","Safety / LSA / FFA","Equipment Related,External Factors,Human Error,Inappropriate Procedure","10.33","High","","","System to be checked and rectified.","2021-10-07T23:59:35","","Completed","2021-08-29T23:59:35","No","No","No","Internal"]
[null,null,null,20730,null,"57_26/8/2021 12:28:41 PM","2021-07-08T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","M2 and M3 winches to derust and paint.","Deck - Mooring Machinery","General Appearance","External Factors","9.14","Medium","","","Derusting & Painting of winches carried out.","2021-09-13T23:59:35","","Completed","2021-08-18T23:59:35","No","No","No","Internal","Update progress in weekly deck maintenance report."]
[null,null,null,20732,null,"57_26/8/2021 12:30:49 PM","2021-07-08T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Pipe supports forward of no:5 COT have spot rusts.","Deck - Pipe / Fittings","General Appearance","External Factors","11.7","High","","","Dersuting carried out.","2021-11-28T23:59:35","","Completed","2021-09-29T23:59:35","No","No","No","Internal","Update progress in weekly deck maintenance report."]
[null,null,null,20415,null,"57_15/8/2021 1:37:59 AM","2021-08-07T23:59:35","Defect","Ship Staff","Ship Staff Insp.","IN S/G ROOM HIGH PRESSURE CLEANING EQUIPMENT SAFETY VALVE LEAKING.","Deck - Machinery","Eng. / Strg. Comp.","Behaviour Based,Equipment Related,External Factors,Inappropriate Procedure","10.32","Very High","","","Valve Received and Renewed.","2021-12-29T23:59:35","DSTA210170","Completed","2021-11-23T23:59:35","No","No","No","Internal","Noted, will process requisition."]
[null,null,null,20736,null,"57_29/8/2021 5:28:18 AM","2021-08-26T23:59:35","Defect,Observation","Ship Staff","Ship Staff Insp.","HFO PFR #1 Pump Mech seal leaking for oil.","E/R - Pumps","Eng. / Strg. Comp.","Behaviour Based,Equipment Related,External Factors,Inappropriate Procedure","10.32","Very High","","","Seal to be renewed.","2021-09-28T23:59:35","DSTA210181","Completed","2021-09-02T23:59:35","No","No","No","Internal","Noted, will supply required spares."]
[null,null,null,20841,null,"57_10/9/2021 6:40:03 PM","2021-09-02T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Ballast valve BA417 found inoperative from CCR panel","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.3","Very High","","","IS power supply repaired behind CCR panel,V/V operating from CCR Panel.","2021-12-02T23:59:35","","Completed","2021-09-12T23:59:35","No","No","No","Internal"]
[null,null,null,20842,null,"57_10/9/2021 6:42:12 PM","2021-09-02T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Cargo Valve CL 228 inoperative from CCR panel","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.3","Very High","","","IS power supply renewed behind CCR panel, V/V tried out ,operating from normally from ccr panel.","2021-12-02T23:59:35","","Completed","2021-09-13T23:59:35","No","No","No","Internal"]
[null,null,null,19980,null,"57_28/6/2021 9:41:55 PM","2021-09-03T23:59:35","Defect,Observation","Ship Staff","Ship Staff Insp.","ME FO CIRCULATING PUMP #1 FRONT COVER IN DAMAGE CONDITION","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related,Human Error,Inappropriate Procedure,Knowledge Based","10.32","Very High","","","Spares Received and overhauled the pump ,tried out found satisfactory.","2021-12-29T23:59:35","DSTA210132/2","Completed","2021-11-23T23:59:35","No","No","No","Internal","PO issued. Waiting spare readiness- Lead time 21 days."]
[null,null,null,21334,null,"57_30/9/2021 10:42:16 PM","2021-09-03T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Enclosed gear oil for Mooring winch M2 & M4 found emulsified during 6M routine of all winches as per PMS.","Deck - Mooring Machinery","Mooring","Equipment Related","9.14","Medium","","","Gear oil for mooring winches M2 & M4 renewed.","2021-11-29T23:59:35","","Completed","2021-09-14T23:59:35","No","No","No","Internal"]
[null,null,null,20412,null,"57_27/7/2021 8:56:56 AM","2021-09-03T23:59:35","Observation","Ship Staff","Nav Audit / Verification","BRIDGE WINDOW WIPER TWIN BLADE DRIVING PCB MODULE MALFUNCTIONING,INDICATING FAULT LED.","Navigation - Others","Navigation","Equipment Related,External Factors,Inappropriate Procedure","4.7","High","","","PCB to be renewed.","2022-01-29T23:59:35","DSTA210156","Completed","2022-01-03T23:59:35","No","No","No","Internal","Noted."]
[null,null,null,21337,null,"57_30/9/2021 10:49:53 PM","2021-09-06T23:59:35","Critical Equipment,Observation","Ship Staff","Ship Staff Insp.","sampling point for Fixed gas detection system for fpk wb tank acess trunk giving flow fault alarm ","Deck - Machinery,Deck - Pipe / Fittings","Safety / LSA / FFA","Equipment Related","5.17","Very High","","","Online filters for sampling point opened and cleaned,line blown through with air and reconnected.System tried,working satisfactorily","2021-12-06T23:59:35","","Completed","2021-09-07T23:59:35","No","No","No","Internal"]
[null,null,null,21333,null,"57_20/9/2021 1:55:58 PM","2021-09-18T23:59:35","Observation","Ship Staff","Ship Staff Insp.","BWTS LOOP 1 MOSS FILTER DRAIN SLUDGE PUMP SEAL LEAKING FOR SEA WATER","Cargo Mach.","Cargo / Ballast Systems","Equipment Related,External Factors,Inappropriate Procedure","6.21","High","","","PUMP OVERHAULED AND MECH SEAL RENEWED.","2022-01-29T23:59:35","DSTA210198","Completed","2021-12-28T23:59:35","No","No","No","Internal","Approved PO. Awaiting spare readiness."]
[null,null,null,21335,null,"57_30/9/2021 10:58:43 PM","2021-09-25T23:59:35","Observation","Ship Staff","Ship Staff Insp."," Fire hose box in forecastle area found broken from hinges. ","LSA / FFA","Safety / LSA / FFA","Equipment Related,External Factors","5.38","High","","","Fire hose box hinges repaired and cover fitted back.","2021-12-25T23:59:35","","Completed","2021-09-27T23:59:35","No","No","No","Internal"]
[null,null,null,21336,null,"57_30/9/2021 10:33:11 PM","2021-09-27T23:59:35","Critical Equipment,Observation","Ship Staff","Ship Staff Insp.","Dressor coupling of Fire line found leaking near no. 2 Foam monitor platform","Deck - Pipe / Fittings,LSA / FFA","Safety / LSA / FFA","Equipment Related","5.38","High","","","Dressor coupling opened,pipe area cleaned and gaskets renewed.","2021-12-27T23:59:35","","Completed","2021-09-28T23:59:35","No","No","No","Internal"]
[null,null,null,19780,null,"57_15/6/2021 11:02:33 AM","2021-09-29T23:59:35","Observation","Ship Staff","Ship Staff Insp.","LT COOLER #1 SW INLET VALVE NOT HOLDING FOR SEA WATER.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","VALVE RENEWED.","2021-12-29T23:59:35","","Completed","2021-12-10T23:59:35","No","No","No","Internal","Spare supplied to vessel. Renew at suitable opportunity."]
[null,null,null,25770,null,"57_18/6/2022 7:18:55 PM","2021-10-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","In pump room BWTS Loop PV211 & PV221 valve malfunctioning. PV 221 valve actuator is broken.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","6.21","High","","","All valves checked, found working ","2022-11-28T23:59:35","DSTA220008","Completed","2022-10-26T23:59:35","No","No","No","Internal"]
[null,null,null,20068,null,"57_14/7/2021 9:40:46 AM","2021-10-03T23:59:35","Other","Ship Staff","Ship Staff Insp.","PUMP ROOM ENTRANCE IG MAIN DECK LINE LOCAL PRESSURE GAUGE MALFUNCTIONING.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related,External Factors,Human Error","8.25","Very High","","","RENEWED PRESSURE GAUGE WITH SPARE NEW ONE.","2022-01-29T23:59:35","DSTA210146","Completed","2021-12-27T23:59:35","No","No","No","Internal","Noted. Spare will be supplied at next Singapore call."]
[null,null,null,20413,null,"57_27/7/2021 8:51:53 AM","2021-10-03T23:59:35","Defect,Observation","Ship Staff","Ship Staff Insp.","STBD & PORT HOSE HANDLING CRANE TRANSFER LIGHT (EXd) TEMPER GLASS IS IN BROKEN CONDITION.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related,External Factors,Inappropriate Procedure","8.5","Very High","","","Complete unit Renewed.","2022-01-29T23:59:35","DSTA210162","Completed","2021-12-27T23:59:35","No","No","No","Internal","Noted. Will process requisition."]
[null,null,null,20414,null,"57_15/8/2021 1:41:00 AM","2021-10-03T23:59:35","Defect","Ship Staff","Ship Staff Insp.","PERSONNEL ELEVATOR MAGNETIC SWITCH MALFUNCTIOING ON SUNKEN DECK.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Behaviour Based,Equipment Related,External Factors,Human Error","10.32","Very High","","","Switch to be renewed.","2021-12-29T23:59:35","DTSA210169","Completed","2021-12-07T23:59:35","No","No","No","Internal","Noted. Awaiting quote."]
[null,null,null,19648,null,"57_28/5/2021 8:48:02 PM","2021-10-03T23:59:35","Observation","Ship Staff","Ship Staff Insp.","FRESH WATER SUPPLY STERILISER UNIT FILTER CASING/COVER THREAD WASTED CAUSING WATERL LEAK.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","The filter cover opened and found the the thread PR RECED WITHOUT COMPLETE FILTER,MAIL CORRESPONDANCE IS IN PROGRESS.","2021-12-29T23:59:35","DSTA210099","Completed","2021-12-05T23:59:35","No","No","No","Internal","Spare is ready. Will be supplied at next opportunity."]
[null,null,null,20731,null,"57_29/8/2021 6:00:06 AM","2021-10-03T23:59:35","Critical Equipment","Ship Staff","Ship Staff Insp.","AUTO PILOT MICROTRANSMIITER NIL ROB","Elect. Mach. & Equip.","Navigation","Behaviour Based,Equipment Related,Human Error,Inappropriate Procedure","10.13","Very High","","","SPARE RECEIVED IN SINGAPORE ","2022-01-29T23:59:35","DSTA210148","Completed","2021-12-26T23:59:35","No","No","No","Internal","PO approved. Awaiting readiness."]
[null,null,null,20734,null,"57_25/8/2021 12:04:00 PM","2021-10-03T23:59:35","Defect,Observation","Ship Staff","Ship Staff Insp.","BWTS PLANT LOOP 2 TRO UNIT MALFUNCTIONAL.","Cargo Mach.,Elect. Mach. & Equip.","Cargo / Ballast Systems","Equipment Related,External Factors,Human Error,Inappropriate Procedure","6.21","High","","","COMPLETE TRO UNIT RECEIVED.","2022-01-29T23:59:35","DSTA215061","Completed","2021-12-26T23:59:35","No","No","No","Internal","Noted. Will supply PCB with optical sensor."]
[null,null,null,20735,null,"57_29/8/2021 5:38:53 AM","2021-10-03T23:59:35","Observation","Ship Staff","Ship Staff Insp.","AUX ENGINE #3 INDICATOR GLASS BROKEN AND PR GAUGES ARE OPAQUE","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related,External Factors,Human Error,Inappropriate Procedure","10.32","Very High","","","NEED TO BE RENEWED.","2022-01-29T23:59:35","DSTA210180","Completed","2021-12-27T23:59:35","No","No","No","Internal","Noted. PO approved. Awaiting readiness."]
[null,null,null,20733,null,"57_31/8/2021 5:15:58 AM","2021-10-08T23:59:35","Observation","Ship Staff","Ship Staff Insp.","BWTS C2E CELL VALVE ACTUATOR AIR HOSES AND CONNECTORS LEAKING FOR AIR.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related,External Factors,Human Error","6.21","High","","","Vessel received the PO but all hoses are silicon type and not fixing in the snap up connectors.At present we are installing additional parallel connectors for arresting the air leakages.","2022-01-29T23:59:35","DSTA210171","Completed","2021-11-28T23:59:35","No","No","No","Internal","Noted. Will process requisition."]
[null,null,null,22487,null,"57_31/10/2021 9:50:50 PM","2021-10-20T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Exhaust valve from AUS drain tank to slop port found frozen and not operable.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.21","High","","","Valve was opened and renewed with spare valve.","2022-01-20T23:59:35","","Completed","2022-10-21T23:59:35","No","No","No","Internal"]
[null,null,null,22488,null,"57_31/10/2021 9:56:45 PM","2021-10-23T23:59:35","Critical Equipment","Ship Staff","Ship Staff Insp.","COW root valve for 3 centre COT was observed to be giving leaking sound even after being closed during cow operations. ","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.34","High","","","Valve was opened after departure port and found that the gear box was wrongly fitted and valve disc was in open position when indication showed fully closed.Valve gearbox repaired & fitted back.","2022-01-23T23:59:35","","Completed","2021-10-26T23:59:35","No","No","No","Internal"]
[null,null,null,22486,null,"57_31/10/2021 1:56:31 AM","2021-10-28T23:59:35","Defect,Observation","Ship Staff","Ship Staff Insp.","MAIN SEA WATER PUMP #2 PUMP SLIGHTELY LEAKING FROM MECH SEAL.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related,External Factors,Human Error,Inappropriate Procedure","10.32","Very High","","","PUMP OVERHAULED.","2022-01-29T23:59:35","DTSA210187","Completed","2021-12-27T23:59:35","No","No","No","Internal","Noted. Rectify leak upon receipt of spares."]
[null,null,null,22691,null,"57_15/11/2021 3:43:05 PM","2021-11-12T23:59:35","Defect","Ship Staff","Ship Staff Insp.","1C COW MACHING POS.94 GEAR SHAFT AND BEARING WERE IN DAMAGED CONDITION,4C COW MACHINE POS 151 PULL ROD LIFT BY APPROX.60-70 MM.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related,External Factors,Human Error,Inappropriate Procedure","8.34","High","","","1C COW MACHINE BEARING AND SHAFT EASED UP AND ASSEMBLED,WORKING SATISFACTORY,4 C COW MACHINE INFORM TO OFFICE FOR FURTHER TROUBLESHOOTING.","2022-01-29T23:59:35","DSTA210236","Completed","2021-12-27T23:59:35","No","No","No","Internal","Requisition approved. Spares will be connected next convenient port."]
[null,null,null,23641,null,"57_5/1/2022 5:23:54 PM","2021-12-30T23:59:35","Defect","Ship Staff","Ship Staff Insp.","ELEVATOR CAR DOOR SPEAKER MALFUNCTIOINING.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related,External Factors,Inappropriate Procedure","10.32","Very High","","","SPEAKERs renewed","2022-11-28T23:59:35","DSTA220007","Completed","2022-08-31T23:59:35","No","No","No","Internal"]
[null,null,null,23642,null,"57_5/1/2022 5:21:06 PM","2021-12-31T23:59:35","Defect","Ship Staff","Ship Staff Insp.","BWTS C2E UNIT GAS SEPARATOR UNIT HAD PIN HOLE,COLD WORK CARRIED OUT.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related,External Factors,Inappropriate Procedure","6.22","Medium","","","Permanent repairs done. Complete unit removed from place and completely buffed to check for any other pin hole or extensive pitting. Found none.\n\nPin hole found near the welding seam of the sensor pocket welded. Unit was pressure tested satisfactorily by filling wiith water. Unit fitted back in place.","2022-01-29T23:59:35","","Completed","2022-01-26T23:59:35","No","No","No","Internal","Noted."]
[null,null,null,23643,null,"57_6/1/2022 3:33:08 PM","2021-12-31T23:59:35","Defect,Observation","Ship Staff","Ship Staff Insp.","BWTS LOOP 1 MOSS FILTER SEA WATER INTAKE FLANGE SLIGHTLEY SEEPAGE FOR SEA WATER ON STBD SIDE.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related,External Factors,Inappropriate Procedure","6.22","Medium","","","LEAK RECTIFIED BY TIGHTENING THE FLANGE EVENLY.","2022-03-29T23:59:35","","Completed","2022-03-01T23:59:35","No","No","No","Internal","Noted."]
[null,null,null,23644,null,"57_8/1/2022 10:56:27 AM","2022-01-05T23:59:35","Defect","Ship Staff","Ship Staff Insp.","DECK SEAL OVERBOARD SHIP SIDE VALVE SEIZED IN OPEN POSITION IN PUMP ROOM.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related,External Factors,Inappropriate Procedure","10.31","Very High","","","VALVE TO BE RENEWED.// note: Actually the valve long handle gear mechanism was tight, removed the gear system cleaned and lubricated, also lubrication done on the valve side and now valve is opening and closing correctly, not sized. ","2023-03-29T23:59:35","","Completed","2022-01-22T23:59:35","No","No","No","Internal","Noted."]
[null,null,null,28993,46997,"57_Thu Mar 09 2023 11:33:58 GMT+0800","2022-01-30T23:59:35","Observation","Ship Staff","Nav Audit / Verification","BRIDGE WING RUDDER ANGLE INDICATORS NOT SYNCHRONIZED","Navigation - Others","Navigation","Equipment Related","10.39","High","","","RUDDER ANGLE INDICATERS SYNCHRONIZED PRIOR ARRIVAL NEXT PORT ON 10 FEB 2022.","2022-03-30T23:59:35","","Completed","2022-02-13T23:59:35","No","No","No","Internal"]
[null,null,null,28994,70666,"0_Thu Mar 09 2023 11:43:01 GMT+0800","2022-01-30T23:59:35","Observation","Ship Staff","Nav Audit / Verification","OUTDATED BRIDGE PUBLICATION NOT REMOVED FROM BRIDGE","Navigation - Others","Navigation","Human Error","4.12","Very High","","","PUBLICATION REMOVED FROM BRIDGE.","2022-03-30T23:59:35","","Completed","2022-01-30T23:59:35","No","No","No","Internal"]
[null,null,null,28995,40132,"0_Thu Mar 09 2023 11:50:18 GMT+0800","2022-01-30T23:59:35","Observation","Ship Staff","Nav Audit / Verification","TWO NOS. BRIDGE WINDOW WIPER BLADED CRACKED AND NEED REPLACEMENT.","Navigation - Others","Navigation","Equipment Related","4.6","Medium","","","WINDOW WIPER BLADES RENEWED WITH SPARES ONBOARD. FULL SET OF SPARE BLADES TO BE CARRIED ONBOARD.","2022-03-30T23:59:35","","Completed","2022-01-30T23:59:35","No","No","No","Internal"]
[null,null,null,24832,null,"57_28/3/2022 8:35:20 AM","2022-02-05T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","No.1 AE unit #1 indicator cock leak to rectify","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Leaky indicator cock replaced with overhauled spare","2022-02-12T23:59:35","","Completed","2022-02-12T23:59:35","No","No","No","Internal"]
[null,null,null,24833,null,"57_28/3/2022 8:37:11 AM","2022-02-05T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","No.2 AE leak observed from FO filter to rectify immediately","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Leak rectified by changing the O-ring of the filter","2022-02-06T23:59:35","","Completed","2022-02-06T23:59:35","No","No","No","Internal"]
[null,null,null,24834,null,"57_28/3/2022 8:43:41 AM","2022-02-05T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Replace the AC fresh air suction filter on ‘C’ deck","Accommodation","MLC Related","Equipment Related","5.1","Very High","","","Air suction filter replaced","2022-02-12T23:59:35","","Completed","2022-02-08T23:59:35","No","No","No","Internal"]
[null,null,null,24835,null,"57_28/3/2022 8:28:47 AM","2022-02-05T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Vegetable room door handle hard to open from inside. Lock to be eased up ","Miscellaneous","Safety / LSA / FFA","Equipment Related","11.13","Low","","","Door handle dismantled, riveted properly to the door and made free","2022-03-05T23:59:35","","Completed","2022-02-25T23:59:35","No","No","No","Internal"]
[null,null,null,24836,null,"57_27/3/2022 4:39:54 AM","2022-02-05T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Winch brake wheel manual operation stopped with cable tie, same found missing in few winches ","Deck - Mooring Machinery","Mooring","Behaviour Based,Knowledge Based","9.7","Medium","","","All the missing winch break wheel to be secured for manual operation with cable tie. Cable tie placed in all the missing winches. ","2022-04-18T23:59:35","","Completed","2022-03-23T23:59:35","No","No","No","Internal"]
[null,null,null,24837,null,"57_27/3/2022 4:30:24 AM","2022-02-05T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Loose Steel plates inside F’castle store, need proper securing ","Miscellaneous","ISM Related","Human Error,Inappropriate Procedure","5.11","Low","","","loose plates required to secure in proper place and need to be secured with wire lashing. Secured with wire lashing inside F'peak store. ","2022-04-18T23:59:35","","Completed","2022-03-25T23:59:35","No","No","No","Internal"]
[null,null,null,24838,null,"57_28/3/2022 8:46:38 AM","2022-02-05T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","No. 4 Engine room blower duct drain line choked. Same to be cleared","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Drain line removed cleared of rust and fitted back","2022-03-05T23:59:35","","Completed","2022-02-28T23:59:35","No","No","No","Internal"]
[null,null,null,24827,null,"57_27/3/2022 4:34:28 AM","2022-02-05T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Spot rust observed in cable holding metal tray securing U-bolt, need maintenance","Deck - Pipe / Fittings","General Appearance","Industry Issue","11.4","Very High","","","De-rusting and painting job to carry out. Work in progress. Work completed. ","2022-05-05T23:59:35","","Completed","2022-04-27T23:59:35","No","No","No","Internal"]
[null,null,null,24831,null,"57_28/3/2022 8:32:25 AM","2022-02-05T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","All AE’s exhaust seal pot filled with carbon. Same to be cleaned, painted and filled with water","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Seal pot drained, cleaned of scale and carbon, painted and filled with fresh water","2022-03-05T23:59:35","","Completed","2022-02-28T23:59:35","No","No","No","Internal"]
[null,null,null,25774,null,"57_18/6/2022 7:35:47 PM","2022-03-01T23:59:35","Defect,Observation","Ship Staff","Ship Staff Insp.","Navigation lights (Stbd sub, Port main and sub, Stern sub, Fore Mast head main & sub) are giving power failure alarm on the navigation light control panel","Navigation - Others","Navigation","Equipment Related","4.8","Medium","","","lights replaced","2022-11-28T23:59:35","DSTA220059 - Navigation Light Spares","Completed","2022-08-30T23:59:35","No","No","No","Internal"]
[null,null,null,24828,null,"57_4/4/2022 8:55:14 AM","2022-03-14T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Port Life/Rescue boat winch Emergency stop switch found not operating due to the shunt coil of the contactor burnt.","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.29","High","","","switch replaced with new spare","2022-11-28T23:59:35","DSTA220066- LIFE/RESCUE BOAT WINCH ELECTRICAL SPARES","Completed","2022-04-04T23:59:35","No","No","No","Internal"]
[null,null,null,24830,null,"57_16/4/2022 9:55:00 AM","2022-04-12T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Temperature controller for ME Scavenge air cooler not working","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","temporary cleaning of pilot valve carried out. ","2022-10-29T23:59:35","DSTA220103 - CONTROL VALVES IN ENGINE ROOM","Completed","2022-10-28T23:59:35","No","No","No","Internal"]
[null,null,null,25775,null,"57_18/6/2022 7:38:54 PM","2022-05-31T23:59:35","Defect","Ship Staff","Ship Staff Insp.","During inspection to ascertain heavy weather damage (from 31-May-2022 to 01-Jun-2022 ), found fire hose box near f'castle area broken. Vessel do not have spare fire hose box onboard.","LSA / FFA","Safety / LSA / FFA","Equipment Related,External Factors","","","","","New hose box received and fitted in place","2022-07-29T23:59:35","DSTA220113","Completed","2022-06-30T23:59:35","No","No","No","Internal"]
[null,null,null,25776,null,"57_18/6/2022 7:47:21 PM","2022-06-02T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Accomodation gas detection system O2 detector malfunctioning","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","8.3","Very High","","","replaced","2022-10-29T23:59:35","DSTA220111 - Oxygen detector for Accomodation gas detection system.","Completed","2022-08-30T23:59:35","No","No","No","Internal"]
[null,null,null,26021,null,"57_30/6/2022 9:32:27 PM","2022-06-23T23:59:35","Defect","Ship Staff","Ship Staff Insp.","O2 analyser #1 showing ‘Sensor Heating’ alarm. Oxygen Probe is defective","Inert Gas","Cargo / Ballast Systems","Equipment Related","8.25","Very High","","","Recieved item, renewed sensor and tested working good.","2022-09-28T23:59:35","DSTA220095 - INERT GAS OXYGEN ANALYSER O2 SENSOR PROBE. DSTA220121- IGS OXYGEN ANALYSER","Completed","2022-08-29T23:59:35","No","No","No","Internal"]
[null,null,null,26158,null,"57_5/7/2022 11:49:21 PM","2022-07-03T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","BWTS EMI filters fitted on the rectifier unit needs to be removed for safety reasons as per maker. EMI filter for 1 unit has been removed and connections done as per manual. Remaining 2 units do not remove the EMI filters as leave it as it is. EMI filters to be renewed upon receipt of new ones as per message from office","Miscellaneous","Cargo / Ballast Systems","Equipment Related","","","","","EMI filter received at Singapore on 29 August 2022 and renewed. Tried out and found satisfactory.","2022-11-28T23:59:35","","Completed","2022-09-26T23:59:35","No","No","No","Internal"]
[null,null,null,26159,null,"57_15/7/2022 4:47:25 PM","2022-07-06T23:59:35","Defect","Ship Staff","Ship Staff Insp.","While mooring operation Electric motor no 1 for Aft hydraulic power was triping due to activation of overload trip.","Deck - Mooring Machinery","Eng. / Strg. Comp.","Equipment Related","","","","","Motor insulation checked. After resetting,motor started and amp checked on individual phase. Suspecting overload trip malfunctioning.","2022-10-05T23:59:35","DSTA220124","Completed","2022-08-31T23:59:35","No","No","No","Internal"]
[null,null,null,26162,null,"57_15/7/2022 1:37:58 AM","2022-07-07T23:59:35","Observation","Ship Staff","Ship Staff Insp.","DH contamination alarm activated for unit no 2 oil mist detector.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Temp of unit checked and confirmed that it was a fault alarm. Sensor cleaned and alarm reseted.","2022-07-08T23:59:35","","Completed","2022-07-08T23:59:35","No","No","No","Internal"]
[null,null,null,27023,null,"57_16/9/2022 2:45:23 PM","2022-07-07T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","Service air compressor colling fan hub was broken and same damaged the fan as well. ","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.1","Medium","","","Spare received at last call Singapore. Fan and Hub was renewed with new spare and tried out. Working satisfactorily.","2022-09-08T23:59:35","","Completed","2022-09-04T23:59:35","No","No","No","Internal"]
[null,null,null,26160,null,"57_15/7/2022 1:27:36 AM","2022-07-08T23:59:35","Defect","Ship Staff","Ship Staff Insp.","O2 detector near IG Blower area malfunctioning","Inert Gas","Eng. / Strg. Comp.","Equipment Related","8.3","Very High","","","New 2 detector received via PO number DSTA220111. O2 detector renwed, same found operational.","2022-11-28T23:59:35","DSTA220111","Completed","2022-11-22T23:59:35","No","No","No","Internal","Noted."]
[null,null,null,26161,null,"57_15/7/2022 4:56:00 PM","2022-07-12T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Stbd Side Pilot Ladder:Observed rope damages developing at 12m step in vicinity of PTR seizing mechanical clamps.Almost 50% of 1 complete strand damaged by mechanical clamp on both sides of step.Total 14 Step fixtures of the ladder was found in damaged condition.","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.47","Medium","","","replaced","2022-10-13T23:59:35","DSTA220130","Completed","2022-08-31T23:59:35","No","No","No","Internal"]
[null,null,null,26479,null,"57_1/8/2022 8:53:43 PM","2022-07-21T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Ballast water treatment system C2E unit 2 hydrogen purge valve found not venting.Hence acting like a accumulator, and causing low level in the c2e unit and erratic pressure pulses in the system which has led to high back pressure on the rectifier. This was not allowing the system to operate properly in auto mode, causing gas lock in the system, and erratic behaviour of the flow meteters and pressure sensors .","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","Temporary purge valve fitted. Both purge valves to be renewed after receiving spares.","2022-11-28T23:59:35","DSTA220128","Completed","2022-11-10T23:59:35","No","No","No","Internal"]
[null,null,null,26638,null,"57_20/8/2022 9:40:33 AM","2022-08-03T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Alarms activating on pump room Gas detection system for analysing and transport pumps.","Hull & Tanks,Miscellaneous","Cargo / Ballast Systems","Equipment Related","","","","","sampling pump overhaul","2022-10-29T23:59:35","DSTA220003","Completed","2022-09-06T23:59:35","No","No","No","Internal"]
[null,null,null,26639,null,"57_20/8/2022 9:47:56 AM","2022-08-04T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Bwts hydrogen blower changeover flap found broken.","E/R - Aux. Mach.","Cargo / Ballast Systems","Equipment Related","","","","","Flap repaired and fitted back.","2022-08-29T23:59:35","","Completed","2022-08-05T23:59:35","No","No","No","Internal"]
[null,null,null,26640,null,"57_20/8/2022 9:36:25 AM","2022-08-16T23:59:35","Defect","Ship Staff","Ship Staff Insp.","During N2 pressure check of accumulators found NO2 unit port accumulator press low and leaking.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Accumulator replaced with overhauled one.","2022-08-29T23:59:35","","Completed","2022-08-16T23:59:35","No","No","No","Internal"]
[null,null,null,26641,null,"57_20/8/2022 9:42:20 AM","2022-08-17T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Engine room crane slow and high speed up/down not working.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","During investigation found brake wire got short. Spare cable used and problem rectified.","2022-10-29T23:59:35","","Completed","2022-08-17T23:59:35","No","No","No","Internal"]
[null,null,null,27710,72343,"57_Sun Nov 20 2022 17:41:59 GMT+0800","2022-08-27T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","VRCS hydraulic lines on deck needs derusting and painting","Deck - Pipe / Fittings","General Appearance","External Factors","11.4","Very High","","","Derusting and painting of VRCS hydraulic lines on deck has been completed.","2022-12-29T23:59:35","","Completed","2022-10-26T23:59:35","No","No","No","Internal","Update progress in weekly deck maintenance report"]
[null,null,null,28996,26868,"0_Thu Mar 09 2023 11:56:14 GMT+0800","2022-08-27T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Nav Audit / Verification","Arrival time at WPT not mentioned in Passage plan from Angra Dos Reis to Zhoushan.","Navigation - Others","Navigation","Human Error","4.20","Very High","","","Arrival time of all waypoints from GPS log & Deck log book was copied to the passage plan waypoint sheet to maintain passage plan execution record.","2022-11-27T23:59:35","","Completed","2022-09-05T23:59:35","No","No","No","Internal"]
[null,null,null,28997,23485,"0_Thu Mar 09 2023 12:07:13 GMT+0800","2022-08-27T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Nav Audit / Verification","BNWAS On/Off entries at Berth not mentioned in Deck log book or Bridge note book for last call at Zhoushan and Tianjin.","Navigation - VDR / BNWAS","Navigation","Human Error","4.7","High","","","Missing entries regarding BNWAS On/Off timings & position were immediately updated in deck logbook & bridge movement book.\nOOWs briefed accordingly.","2022-11-27T23:59:35","","Completed","2022-09-05T23:59:35","No","No","No","Internal"]
[null,null,null,28998,82193,"0_Thu Mar 09 2023 12:02:43 GMT+0800","2022-08-27T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Nav Audit / Verification","Safety contour settings mentioned in Passage plan from Angra Dos Reis to Zhoushan was incorrect for Open Seas.","Navigation - Others","Navigation","Inappropriate Procedure","4.20","Very High","","","The Passage plan sheet UKC column was updated for safety contour settings in open sea passage legs with min UKC 50% of vessel's static draft.\nNavigating officers were briefed accordingly to ensure safety contour settings in Open sea legs comply with UKC policy.","2022-11-27T23:59:35","","Completed","2022-09-05T23:59:35","No","No","No","Internal"]
[null,null,null,28524,77493,"57_Tue Jan 17 2023 19:42:00 GMT+0800","2022-08-27T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","220V Insulation level at 3 M Ohm. ETO to find out and rectify earth fault.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.38","Medium","","","Insulation checks carried out by isolating one by one section. Found one of the crew cabin equipment with low insulation. same has been isolated and removed from socket. Insulation level increased close to infinity","2022-11-26T23:59:35","","Completed","2022-09-12T23:59:35","No","No","No","Internal"]
[null,null,null,28525,60807,"57_Tue Jan 17 2023 21:42:47 GMT+0800","2022-08-27T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Both O2 sensors for IG platforms defective","Inert Gas","Eng. / Strg. Comp.","Equipment Related","8.30","High","","","New O2 sesnor received at Linggi, Malaysia. Sensor renewed and calibrated, found operational.","2022-11-26T23:59:35","","Completed","2022-11-22T23:59:35","No","No","No","Internal"]
[null,null,null,28526,59783,"57_Tue Jan 17 2023 22:05:09 GMT+0800","2022-08-27T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","PV valve mesh – spare requisition to raise","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.41","Medium","","","All PV valve wire mesh renewed in drydock and fitted back","2022-10-26T23:59:35","","Completed","2023-04-13T23:59:35","No","No","No","Internal"]
[null,null,null,28527,35099,"57_Tue Jan 17 2023 21:59:35 GMT+0800","2022-08-27T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","PV valve test bench size not matching with vessel’s PV valve. New adaptor flange of matching size to supply","Inert Gas","Cargo / Ballast Systems","Equipment Related","8.41","Medium","","","Adaptor flange for PV valve test bench received under DSTA225057","2022-11-26T23:59:35","","Completed","2023-03-02T23:59:35","No","No","No","Internal"]
[null,null,null,28528,83988,"57_Tue Jan 17 2023 21:36:47 GMT+0800","2022-08-27T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Port Windlass clutch valve assembly defective","Deck - Mooring Machinery","Mooring","Equipment Related","9.20","Medium","","","Spare valve block received under DSTA220162, new valve block fitted in place. Port WIndlass operated for correct operation.Noted found in working condition.","2022-11-26T23:59:35","","Completed","2023-04-14T23:59:35","No","No","No","Internal"]
[null,null,null,28529,15609,"57_Tue Jan 17 2023 19:38:16 GMT+0800","2022-08-27T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Hull Markings- Port and Stbd draft marks faded.","Hull & Tanks","General Appearance","External Factors","11.2","Medium","","","Fwd & aft draft marks painted in drydock.","2023-04-24T23:59:35","","Completed","2023-04-15T23:59:35","No","No","No","Internal"]
[null,null,null,28530,98377,"57_Tue Jan 17 2023 21:52:47 GMT+0800","2022-08-27T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","4P ballast tank level gauge defective","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.13","Medium","","","During laden passage inspection of adjacent ballast tanks carried out. Pnuematic piping system for remote gauging inspection carried out. Found minor leak in the air supply in the flanges. Loose nut & bolts for the flanges tightened. Same under observation. ","2022-10-26T23:59:35","","Completed","2022-10-24T23:59:35","No","No","No","Internal"]
[null,null,null,28531,76758,"57_Tue Jan 17 2023 22:13:25 GMT+0800","2022-08-27T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Both Lifeboat gripes- sheathing to remove","LSA / FFA","Safety / LSA / FFA","Inappropriate Procedure","5.27","Medium","","","Both the lifeboats lashing gripes sheathing removed, gripes inspected, no damages observed.","2022-09-26T23:59:35","","Completed","2022-09-06T23:59:35","No","No","No","Internal"]
[null,null,null,27022,null,"57_16/9/2022 4:31:13 PM","2022-09-06T23:59:35","Defect","Ship Staff","Ship Staff Insp.","MAIN ENGINE Variable exhaust gas bypass valve malfunctioning and same was found issue with the SIPART I/P converter controller.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Troubleshooting carried out and found issue with the SIPART controller and office informed and RO DSTA 220167 raised for the same. Vessel received spares at Singapore on 26 Nov 2022. IP Convertor renewed. system tried out found working satisfactory","2022-12-29T23:59:35","DSTA220167","Completed","2022-12-21T23:59:35","No","No","No","Internal","Noted, will process the requisition."]
[null,null,null,28999,58204,"0_Thu Mar 09 2023 12:12:39 GMT+0800","2022-09-18T23:59:35","Observation","Ship Staff","Nav Audit / Verification","Navtex Nav Warnings auto plotting on ECDIS were not verified by OOWs during their respective watch as Navtex message box showed various Navtex messages as unread.","Navigation - Others","Navigation","Human Error","4.13","Very High","","","Bridge Team meeting was conducted to address the observation. Practice put in place that every OOW will check all Navtex messages during his watch and verify that applicable warnings are plotted on ECDIS. Relieving OOW will verify same as part of his takeover routine. All Navtex messages in ECDIS inbox must be acknowledged to shows as Read.  Consequences of missing out Navtex Navigational warnings discussed.","2022-12-18T23:59:35","","Completed","2022-10-10T23:59:35","No","No","No","Internal"]
[null,null,null,29000,94381,"0_Thu Mar 09 2023 12:16:53 GMT+0800","2022-09-18T23:59:35","Observation","Ship Staff","Nav Audit / Verification","Alteration of course was not logged down in deck log book on few occasions.","Navigation - Others","Navigation","Human Error","4.2","Medium","","","Missing log entries completed by respective OOW. Bridge Team meeting was conducted and all OOWs instructed to ensure all course alterations recorded in deck log book in addition to GPS log.","2022-12-18T23:59:35","","Completed","2022-10-10T23:59:35","No","No","No","Internal"]
[null,null,null,27711,36502,"57_Sun Nov 20 2022 19:34:17 GMT+0800","2022-11-04T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Aux Boiler No 1 feed water controller valve found getting stuck. ","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Feed water valve removed, spindle cleaned. Controller calibration carried out. Valve tried out found working satisfactory","2022-11-08T23:59:35","","Completed","2022-11-05T23:59:35","No","No","No","Internal"]
[null,null,null,27795,43775,"57_Thu Dec 01 2022 07:14:48 GMT+0800","2022-11-16T23:59:35","Defect","Ship Staff","Ship Staff Insp.","No. 3 COP seperator level gauge  in CCR found showing erratic readings.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.8","Medium","","","New level transmitter fitted in drydock and calibrated by HKT service engineer","2023-02-15T23:59:35","DSTA220233","Completed","2023-04-03T23:59:35","No","No","No","Internal","Noted. PO approved for spare transmitter, awaiting readiness."]
[null,null,null,27799,16433,"57_Thu Dec 01 2022 07:58:07 GMT+0800","2022-11-16T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Steering gear autopilot system activating \"No 1 servo loop fail alarm \" on rudder command of hard stbd in hand steering mode","Critical Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Checks carried out found feedback signal from the no 1 unit system is not matching to actual rudder position. Service Engineer attended the vessel on 26 Nov 2022 at Singapore. Potentio meter renewed. System tried out found working satisfactory.","2022-11-28T23:59:35","","Completed","2022-11-24T23:59:35","No","No","No","Internal"]
[null,null,null,27974,78013,"57_Wed Dec 21 2022 00:58:17 GMT+0800","2022-11-22T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Few Garbage bins pedestal lid opening mechanism found not working","Miscellaneous","General Appearance","Equipment Related","6.20","Medium","","","Damaged / inoperational lid opening garbage bins have been discarded, new bins have been colour coded and stencilled for garbage category and placed in the respective locations.","2023-01-06T23:59:35","","Completed","2022-11-28T23:59:35","No","No","No","Internal"]
[null,null,null,27793,11518,"57_Thu Dec 01 2022 07:37:27 GMT+0800","2022-11-22T23:59:35","Observation,Non Conformity","Ship Staff","Ship Staff Insp.","During routine lift check of PV valves prior arrival port, 3S vacuum side found to be slightly leaking. Same also verified by placing a personal gas meter around the flame screen of vacuum side.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.19","High","","","3S PV valve was inspected, cleaned and overhauled. Vacuum seat & disc lapped. Pressure testing carried out. Same fitted back and tested using a personal gas meter around the pressure side cone & vacuum side, no leaks noted.","2022-12-21T23:59:35","","Completed","2022-11-28T23:59:35","No","No","No","Internal","Noted."]
[null,null,null,27796,47675,"57_Thu Dec 01 2022 06:28:42 GMT+0800","2022-11-22T23:59:35","Observation","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","The duty engineers were issued two beer cans each on 28th and 29th\nOctober 2022 as per the beer consumption log and carried out night rounds from 2100 hours till 2200 hours as per the rest hour records. As per the company policy, no beers were to be issued for watchkeepers 5 hours before their watches, however, the beers were issued during dinner time.","Documentation","Crew Management","Human Error","3.8","Very High","","","Notice has been posted in the officer's & crew's recreation room stating Company's Alcohol Policy, \"No beer will be issued to watchkeepers 5 hours prior to thier scheduled watch\".\nIt was noted and confirmed during the investigation that this has been an isolated clerical error by the officer in charge in maintaining the beer consumption log.\nDuring vessel’s call at Singapore on 26 Nov 2022, both Marine and Technical Superintendents boarded the vessel and a thorough investigation was carried out regarding this matter. The beer consumption log was checked and compared with the actual inventory of beer cans on board and confirmed that no beer cans were unaccounted for.  Additionally, a thorough\ninterview of all ship staff was carried out to verify that there was no violation of the company’s alcohol policy.","2022-11-28T23:59:35","","Completed","2022-11-24T23:59:35","No","No","No","External"]
[null,null,null,27797,80315,"57_Thu Dec 01 2022 06:49:00 GMT+0800","2022-11-22T23:59:35","Observation","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","The port and starboard bilge suction valves at the pumproom bottom were noted in a shut position. It was immediately opened after being pointed out.","Cargo Mach.","Cargo / Ballast Systems","Inappropriate Procedure","8.47","Very High","","","During the voyage to disport the routine overhauling of the pump room bilge non-return suction valves CL 181 and CL 182 was carried out on 22 Nov 2022. On completion of the same, valves CL 181 and CL 182 were inadvertently left in the closed position. Upon being pointed out, both valves CL 181 and CL 182 were\nimmediately opened. Notices stating, “Keep this suction valve\nopen at all times” and “Do not operate without Ch. Officer's permission” have been posted in the vicinity of valves CL 181 and CL 182","2022-11-28T23:59:35","","Completed","2022-11-22T23:59:35","No","No","No","External"]
[null,null,null,27798,98365,"57_Thu Dec 01 2022 06:57:37 GMT+0800","2022-11-22T23:59:35","Observation","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","The draft marks on the port side were noted not clearly legible between the water level to anti-fouling marking area on the forward perpendicular, between 13.5 meters of water level to 16 meters on the midship area and between 16 meters to 20 meters on the aft perpendicular.","Hull & Tanks","General Appearance","External Factors","11.2","Medium","","","The 3 monthly inspections of the Hull and Loadline Marks were carried out by the ship staff in Singapore during bunkering on 29 Aug 2022. The load line marks were touched up by the ship staff as needed during this time.  The vessel has been engaged on long voyages for the past 3 months from Brazil to China and West Africa to China with no suitable opportunity to arrange\nthe inspection or painting of the draft marks.  ","2023-02-21T23:59:35","","Completed","2022-11-25T23:59:35","No","No","No","External"]
[null,null,null,27968,19071,"57_Wed Dec 21 2022 00:34:22 GMT+0800","2022-11-23T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Spot scattered rust observed on the port side provision crane","Deck - Machinery","General Appearance","Equipment Related","11.8","Low","","","Derusting, power tooling, primer and final coat stripe painting carried out on the port side provision crane.","2023-01-06T23:59:35","","Completed","2022-12-05T23:59:35","No","No","No","Internal"]
[null,null,null,27969,99821,"57_Wed Dec 21 2022 00:36:47 GMT+0800","2022-11-23T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Spot scattered rust observed on the port side lifeboat davit","LSA / FFA","General Appearance","Equipment Related","11.8","Low","","","Derusting, power tooling, primer and stripe final coat application carried out on the port side lifeboat davit. ","2023-01-06T23:59:35","","Completed","2022-12-05T23:59:35","No","No","No","Internal"]
[null,null,null,27970,25083,"57_Wed Dec 21 2022 00:40:06 GMT+0800","2022-11-23T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Rust weeping marks observed on swimming pool & accommodation block window glasses edges.","Accommodation","General Appearance","External Factors","11.8","Low","","","Derusting, power tooling, primer and stripe final coat application carried out on the accommodation block & swimming pool funnel block window glasses edges","2023-01-06T23:59:35","","Completed","2022-12-07T23:59:35","No","No","No","Internal"]
[null,null,null,27971,94290,"57_Wed Dec 21 2022 00:44:12 GMT+0800","2022-11-23T23:59:35","Observation","Owner / Marine / Tech. Suptd.","ISM Audit","IMO symbol & stencil marking on Foam hose box at brake of accommodation found faded","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.15","Medium","","","New stencilling carried out & new IMO symbol posted on the foam hose boxes at the break of accommodation.","2022-12-22T23:59:35","","Completed","2022-11-28T23:59:35","No","No","No","Internal"]
[null,null,null,27972,84449,"57_Wed Dec 21 2022 00:55:20 GMT+0800","2022-11-23T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Mooring winches hydraulic brakes adjustment wheel restraining straps found broken on few winches. ","Deck - Mooring Machinery","Mooring","Equipment Related","9.14","Medium","","","New restraining straps (cable ties) fitted on the mooring winch & windlass hydraulic brake adjustment wheel.","2022-12-22T23:59:35","","Completed","2022-11-28T23:59:35","No","No","No","Internal"]
[null,null,null,27975,29556,"57_Wed Dec 21 2022 01:01:45 GMT+0800","2022-11-23T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Stbd. Bridge wing sliding door not locking in closed position.","Accommodation","ISPS Related","Equipment Related","5.10","High","","","The locking mechanism was found to be damaged, same replaced with new spare lock available onboard. Door and locking mechanism tested, found operational.","2023-02-22T23:59:35","","Completed","2022-12-09T23:59:35","No","No","No","Internal"]
[null,null,null,28212,32332,"57_Wed Dec 28 2022 23:23:18 GMT+0800","2022-11-24T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","LT Cooler sea water line temperature transmitter has minor leak","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.36","Very High","","","Job carried out during docking, leak rectified.","2023-03-29T23:59:35","","Completed","2023-04-12T23:59:35","No","No","No","Internal","Plan to rectify this defect during next anchorage."]
[null,null,null,28213,23553,"57_Thu Dec 29 2022 00:02:41 GMT+0800","2022-11-24T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ER casing has scattered rust spots on port & stbd sides and Aft.","Hull & Tanks","General Appearance","External Factors","11.8","Low","","","Port and stbd side scattered rust has been power tooled, primered and stripe painted with finish coat. \n","2023-02-23T23:59:35","","Completed","2023-03-12T23:59:35","No","No","No","Internal","Update status in weekly deck maintenance report."]
[null,null,null,28214,48113,"57_Thu Dec 29 2022 00:06:16 GMT+0800","2022-11-24T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Windlass brake alignment mark to highlight.","Deck - Machinery","Mooring","Equipment Related","9.20","Medium","","","Highlighted the windlass brake alignment mark in yellow colour on both the windlass.","2022-12-23T23:59:35","","Completed","2022-11-30T23:59:35","No","No","No","Internal"]
[null,null,null,28215,65651,"57_Thu Dec 29 2022 00:04:18 GMT+0800","2022-11-24T23:59:35","Defect","Ship Staff","Suptd. Insp.","Ballast Tank Gas Detection System showing “Compressed Instrument Air” alarm.","Miscellaneous","Cargo / Ballast Systems","Equipment Related","8.46","Very High","","","Fixed gas detection system cabinet for ballast tank inspected, the sampling hose from air filter to solenoid bank was found to be leaking air, pinhole observed caused due to chafing. Sampling hose renewed, system now fully operational with no alarms","2023-01-23T23:59:35","","Completed","2022-11-26T23:59:35","No","No","No","Internal"]
[null,null,null,28216,64707,"57_Wed Dec 28 2022 23:51:31 GMT+0800","2022-11-24T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Stbd Windlass gear oil emulsified","Deck - Mooring Machinery","Mooring","Equipment Related","9.20","Medium","","","Stbd side windlass old gear oil completely drained. New oil refilled upto normal level.","2022-12-24T23:59:35","","Completed","2022-12-14T23:59:35","No","No","No","Internal"]
[null,null,null,28218,37212,"57_Thu Dec 29 2022 00:00:02 GMT+0800","2022-11-24T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ER Foam system valve SSV not in auto position","LSA / FFA","Emgcy. Systems","Equipment Related","5.35","Medium","","","Valve lever put in auto mode","2022-12-24T23:59:35","","Completed","2022-11-24T23:59:35","No","No","No","Internal"]
[null,null,null,27973,30545,"57_Wed Dec 21 2022 01:08:31 GMT+0800","2022-11-24T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Rust weeping marks observed on the IG pipeline near accommodation & funnel block","Accommodation","General Appearance","External Factors","11.8","Low","","","Same de-rusted, primer and stripe final coat applied.","2022-12-23T23:59:35","","Completed","2022-12-14T23:59:35","No","No","No","Internal"]
[null,null,null,27976,26751,"57_Wed Dec 21 2022 01:12:26 GMT+0800","2022-11-24T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Emulsification observed in the stbd windlass gear oil. Oil to be renewed.","Deck - Mooring Machinery","Mooring","External Factors","9.14","Medium","","","Entire stbd side windlass old gear oil drained. New gear oil filled in. Sight glass cleaned and inspected.","2022-12-23T23:59:35","","Completed","2022-12-14T23:59:35","No","No","No","Internal"]
[null,null,null,27966,23714,"57_Tue Dec 20 2022 16:33:53 GMT+0800","2022-12-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","BWTS C2E unit Hydrogen gas separator chamber has developed few pin holes","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Permanenet repair by hotwork to be carried out.\nRO DSTA225087 has been raised from office for new sacrificial anode","2023-03-01T23:59:35","DSTA225087","Completed","2023-02-14T23:59:35","No","No","No","Internal","Noted."]
[null,null,null,27967,86567,"57_Wed Dec 21 2022 00:02:09 GMT+0800","2022-12-05T23:59:35","Observation","Ship Staff","Ship Staff Insp.","All the PV valves fitted to be inspected, cleaned & overhauled. Pressure testing to be carried out with maker's test kit.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.19","High","","","All PV valves overhauled and pressure tested by shipyard and witness by ship's staff.","2023-03-04T23:59:35","","Completed","2023-04-11T23:59:35","No","No","No","Internal","Noted, update progress in weekly deck maintenance report."]
[null,null,null,27977,33816,"57_Tue Dec 20 2022 16:21:20 GMT+0800","2022-12-11T23:59:35","Defect","Ship Staff","Ship Staff Insp.","HFO Bunker line dresser coupling seal found slightly leaking","Deck - Pipe / Fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Sealing gaskets renewed. Bunker line pressure tested . Found all satisfactory","2022-12-18T23:59:35","","Completed","2022-12-11T23:59:35","No","No","No","Internal"]
[null,null,null,27978,59290,"57_Tue Dec 20 2022 16:23:58 GMT+0800","2022-12-13T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","FWG flowmeter found not working","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Flowmeter replaced with new spare flowmeter","2022-12-18T23:59:35","","Completed","2022-12-13T23:59:35","No","No","No","Internal"]
[null,null,null,25772,null,"57_18/6/2022 7:26:17 PM","2022-12-18T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Onboard Flame Detector Tester condition of plastic cup not satisfactory","Elect. Mach. & Equip.","Safety / LSA / FFA","Equipment Related","5.35","Medium","","","Received new flame detector spare under DSTA220161, same tested and confirmed for correct operation.","2023-02-26T23:59:35","DSTA220161 FLAME DETETCTOR SALWICO UV TESTER SET","Completed","2023-03-03T23:59:35","No","No","No","Internal","PO approved, awaiting readiness."]
[null,null,null,28217,70038,"57_Mon Jan 02 2023 00:47:24 GMT+0800","2022-12-24T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Stbd lifeboat engine starting motor found not engaging","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.27","Medium","","","starter motor removed. All parts cleaned. starter tried out. Engine found working satisfactory.","2023-01-25T23:59:35","","Completed","2022-12-24T23:59:35","No","No","No","Internal"]
[null,null,null,24829,null,"57_4/4/2022 9:11:34 AM","2022-12-27T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Main Sea Water Pump #2 leaking from seal. No spare seal onboard","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Pump overhauled with new mech seal, shaft sleeve and line bearing. Pump tried out leak rectified.","2023-02-26T23:59:35","DSTA220029 - Main Cooling Sea Water Pump Spares","Completed","2023-02-12T23:59:35","No","No","No","Internal","PO approved. Awaiting readiness."]
[null,null,null,27794,66894,"57_Mon Nov 21 2022 11:19:42 GMT+0800","2022-12-28T23:59:35","Defect","Ship Staff","Ship Staff Insp.","BWTS rectifier Power supply unit is burnt.","Miscellaneous","Cargo / Ballast Systems","Equipment Related","6.21","High","","","RO raised under DSTA220175 and same renewed..","2023-02-26T23:59:35","","Completed","2023-05-01T23:59:35","No","No","No","Internal","Noted. PO approved, awaiting readiness."]
[null,null,null,28506,73577,"57_Mon Jan 16 2023 02:37:59 GMT+0800","2023-01-10T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Water ballast pump No#1 found leaking from mech seal","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.8","Medium","","","Ballast pump No#1 top mech seal removed from spring stuck due to accumulation of deposits from BWTS catholyte. All parts cleaned. Shaft surface polished. mech seal(except stopper ring54-7) and ball bearing(6316C3) renewed. Pump tried out found working satisfactory","2023-01-14T23:59:35","","Completed","2023-01-11T23:59:35","No","No","No","Internal"]
[null,null,null,28986,16753,"57_Mon Jan 30 2023 15:06:22 GMT+0800","2023-01-22T23:59:35","Defect","Ship Staff","Ship Staff Insp.","CCR panel LED's for valve not showing any indication ","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.8","Medium","","","Power supply unit received, same installed.","2023-04-26T23:59:35","DSTA230005","Completed","2023-03-03T23:59:35","No","No","No","Internal"]
[null,null,null,28987,79460,"57_Wed Feb 15 2023 17:14:44 GMT+0800","2023-02-02T23:59:35","Defect","Ship Staff","Ship Staff Insp.","All COPTs main and steam inlet valves found leaking.","Cargo Mach.","Eng. / Strg. Comp.","Equipment Related","10.36","Very High","","","All valves to be overhauled in DD, specs for the same raised ad exported to office. All valves overhauled duirng DD. Tested the COPT steam system no leaks noted.","2023-03-29T23:59:35","","Completed","2023-04-17T23:59:35","Yes","No","No","Internal"]
[null,null,null,28991,31957,"57_Tue Feb 28 2023 20:52:46 GMT+0800","2023-02-16T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Sanitary exhaust suction found not effective in accommodation spaces.","Deck - Pipe / Fittings","Eng. / Strg. Comp.","Equipment Related","10.30","High","","","Sanitary exhaust fan vent head strainer found clogged , same removed place and cleaned. Vent head boxed back. ","2023-02-26T23:59:35","","Completed","2023-02-18T23:59:35","No","No","No","Internal"]
[null,null,null,28992,69248,"57_Tue Feb 28 2023 21:01:58 GMT+0800","2023-02-23T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Sterilizer current noted deviating from normal,","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.36","Very High","","","Anode found completely wasted upon inspection. Same was renewed with spare. Flow and current adjusted as per instruction manual.","2023-02-26T23:59:35","","Completed","2023-02-23T23:59:35","No","No","No","Internal"]
[null,null,null,29891,52708,"57_Wed Mar 15 2023 09:39:22 GMT+0800","2023-03-11T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Incinerator WO tank 1 & 2 level gauges malfunction","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.36","Very High","","","Gauges renewed with new spare, now both are operational.","2023-03-29T23:59:35","","Completed","2023-04-11T23:59:35","No","No","No","Internal"]
[null,null,null,30239,42035,"57_Mon May 15 2023 19:26:40 GMT+0800","2023-05-07T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Forward bosun store mechanical mushroom vent frozen, unable to close","Deck - Machinery","Structural Condn. / WT integrity ","Equipment Related","","","","","Dismantle and overhaul.","2023-05-13T23:59:35","","Completed","2023-05-12T23:59:35","No","No","No","Internal"]
[null,null,null,30240,45779,"57_Mon May 15 2023 19:22:17 GMT+0800","2023-05-07T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Fire/ Foam Isolation valves on main deck frozen","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","Freeup, Lubrication","2023-05-13T23:59:35","","Completed","2023-05-12T23:59:35","No","No","No","Internal"]
[null,null,null,null,87314,"57_Mon Jan 30 2023 15:26:44 GMT+0800","2023-01-16T08:00:00","Breakdown","Ship Staff","Ship Staff Insp.","Acco A/C Compressor No#1 breakdown due to failure of the unloader device one side spring retainer","Accommodation","MLC Related","Equipment Related","","","","","Spares received under DSTA230048, parts replaced with new spares. Compressor tried out, noted stage #1 not pumping due to indentation marks on suction valve seat, stage #2 pumping, stage #3 not pumping. Due to short cycling of refrigerant in stage #1 & #3, discharge temp goes high and compressor eventually stops on high temp. Compressor was dismantled again for carrying out further checks, noted unloader arms sluggish. Unloader arms freed up and compressor baxed back. Compressor tried out all parameters found normal, same put in service. ","2023-06-29T08:00:00","DSTA230090","Completed","2023-03-25T08:00:00","No","No","No","Internal"]

{"sheet":"Calc","index":2,"n_rows":28,"n_cols":12,"rows_kept":28,"cut":false,"hidden":true,"merged":[]}
["Def_type","Def_cause","Equipments","VIQrefno","Observer_code"]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,"Dim itemSele As Long"]
[null,null,null,null,null,null,null,null,null,null,null,"   dim startRow as integer"]
[null,null,null,null,null,null,null,null,null,null,null,"   startRow=1"]
[null,null,null,null,null,null,null,null,null,null,null,"        For itemSele = 0 To ListBox1.ListCount - 1"]
[null,null,null,null,null,null,null,null,null,null,null,"        If ListBox1.Selected(itemSele) = True Then"]
[null,null,null,null,null,null,null,null,null,null,null,"        Worksheets(\"WorksheetName\").Range(\"A\" & startRow).Value = ListBox1.List(itemSele)"]
[null,null,null,null,null,null,null,null,null,null,null,"        startRow = startRow + 1"]
[null,null,null,null,null,null,null,null,null,null,null,"        End If"]
[null,null,null,null,null,null,null,null,null,null,null,"        Next"]
[null,null,null,null,null,null,null,null,null,null,null,"Dim LastRowA As String"]
[null,null,null,null,null,null,null,null,null,null,null,"        Dim itemSele As Long"]
[null,null,null,null,null,null,null,null,null,null,null,"       Dim startRow as integer"]
[null,null,null,null,null,null,null,null,null,null,null,"        LastRowA = ActiveSheet.Cells(Rows.count, \"A\").End(xlUp).row"]
[null,null,null,null,null,null,null,null,null,null,null,"        startQue = 0"]
[null,null,null,null,null,null,null,null,null,null,null,"        For itemSele = 0 To ListBox1.ListCount - 1"]
[null,null,null,null,null,null,null,null,null,null,null,"        For startRow = 1 To LastRowA"]
[null,null,null,null,null,null,null,null,null,null,null,"        If Worksheets(\"WorksheetName\").Range(\"A\" & startRow).Value = ListBox1.List(itemSele) Then"]
[null,null,null,null,null,null,null,null,null,null,null,"        ListBox1.Selected(itemSele) = True"]
[null,null,null,null,null,null,null,null,null,null,null,"        Exit For"]
[null,null,null,null,null,null,null,null,null,null,null,"        End If"]
[null,null,null,null,null,null,null,null,null,null,null,"        Next j"]
[null,null,null,null,null,null,null,null,null,null,null,"        Next"]
[null,null,null,null,null,null,null,null,null,null,null,"        End If"]

{"sheet":"Areaofobs","index":3,"n_rows":17,"n_cols":2,"rows_kept":17,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Cargo / Ballast Systems",11]
["Cert. & Docu.",2]
["Communication",6]
["Crew Management",3]
["Emgcy. Systems",13]
["Eng. / Strg. Comp.",14]
["General Appearance",15]
["Ice Opns.",17]
["ISM Related",7]
["ISPS Related",10]
["MARPOL Related",9]
["MLC Related",4]
["Mooring",12]
["Navigation",5]
["Safety / LSA / FFA",8]
["Structural Condn. / WT integrity ",16]

{"sheet":"Vessel_type","index":4,"n_rows":1,"n_cols":2,"rows_kept":1,"cut":false,"hidden":true,"merged":[]}
["Vessel_type","ID"]

{"sheet":"Deficiency_type","index":5,"n_rows":8,"n_cols":3,"rows_kept":8,"cut":false,"hidden":true,"merged":[]}
["TITLE","Type of deficiency_description","ID"]
["Breakdown",null,6]
["Critical Equipment",null,4]
["Defect",null,1]
["Guarantee Claim",null,8]
["Non Conformity",null,2]
["Observation",null,3]
["Other",null,7]

{"sheet":"VIQrefno","index":6,"n_rows":427,"n_cols":3,"rows_kept":427,"cut":false,"hidden":true,"merged":[]}
["VIQ_ref_no","Risk Value of observation","ID"]
["1.1","Low",8243]
["1.10","Low",8252]
["1.11","Low",8253]
["1.12","Low",8254]
["1.13","Low",8255]
["1.14","Low",8256]
["1.15","Low",8257]
["1.16","Low",8259]
["1.17","Low",8260]
["1.18","Low",8261]
["1.19","Low",8262]
["1.2","Low",8244]
["1.20","Low",8263]
["1.21","Low",8265]
["1.22","Low",8266]
["1.23","Low",8267]
["1.24","Low",8268]
["1.25","Low",8269]
["1.26","Low",8270]
["1.3","Low",8245]
["1.4","Low",8246]
["1.5","Low",8247]
["1.6","Low",8248]
["1.7","Low",8249]
["1.8","Low",8250]
["1.9","Low",8251]
["1.99","High",11258]
["10.1","Medium",8461]
["10.10","High",8470]
["10.11","Medium",8471]
["10.12","Very High",8472]
["10.13","Very High",8473]
["10.14","Medium",8474]
["10.15","Low",8475]
["10.16","Very High",8476]
["10.17","Very High",8477]
["10.18","High",8478]
["10.19","Very High",8479]
["10.2","Low",8462]
["10.20","High",8480]
["10.21","Medium",8481]
["10.22","Low",8482]
["10.23","Medium",8483]
["10.24","Low",8484]
["10.25","Very High",8485]
["10.26","High",8486]
["10.27","Medium",8487]
["10.28","Low",8488]
["10.29","Medium",8489]
["10.3","Medium",8463]
["10.30","High",8490]
["10.31","Very High",8491]
["10.32","Very High",8492]
["10.33","High",8493]
["10.34","High",8494]
["10.35","Very High",8495]
["10.36","Very High",8496]
["10.37","Medium",8497]
["10.38","Medium",8498]
["10.39","High",8499]
["10.4","High",8464]
["10.40","Medium",8500]
["10.41","Medium",8501]
["10.42","Medium",8502]
["10.43","Medium",8503]
["10.44","Medium",8504]
["10.45","Very High",8505]
["10.46","High",8506]
["10.47","Medium",8507]
["10.48","High",8508]
["10.49","Medium",8509]
["10.5","Low",8465]
["10.50","High",8510]
["10.51","Low",8511]
["10.52","Medium",8512]
["10.53","Medium",8513]
["10.54","High",8514]
["10.55","Low",8515]
["10.6","Very High",8466]
["10.7","Medium",8467]
["10.8","Medium",8468]
["10.9","Medium",8469]
["10.99","High",8516]
["11.1","High",8420]
["11.10","Medium",8429]
["11.11","Very High",8430]
["11.12","Low",8431]
["11.13","Low",8432]
["11.14","Medium",8433]
["11.15","Low",8434]
["11.16","Low",8435]
["11.17","Low",8436]
["11.2","Medium",8421]
["11.3","Medium",8422]
["11.4","Very High",8423]
["11.5","Medium",8424]
["11.6","Medium",8425]
["11.7","High",8426]
["11.8","Low",8427]
["11.9","Low",8428]
["11.99","High",8437]
["12.1","High",8438]
["12.10","High",8448]
["12.11","High",8449]
["12.12","High",8450]
["12.13","High",8451]
["12.14","High",8452]
["12.15","High",8453]
["12.16","High",8454]
["12.17","High",8455]
["12.18","High",8456]
["12.19","High",8457]
["12.2","High",8439]
["12.20","High",8458]
["12.21","High",8459]
["12.3","High",8441]
["12.4","High",8442]
["12.5","High",8443]
["12.6","High",8444]
["12.7","High",8445]
["12.8","High",8446]
["12.9","High",8447]
["12.99","High",8460]
["2.1","Very High",8296]
["2.1.9","Very High",11259]
["2.10","Medium",8304]
["2.11","Medium",8305]
["2.12","Low",8306]
["2.13","Low",8307]
["2.14","Low",8308]
["2.15","Low",8309]
["2.16","Medium",8310]
["2.2","Medium",8297]
["2.3","High",8295]
["2.4","Medium",8298]
["2.5","Medium",8299]
["2.6","Low",8300]
["2.7","High",8301]
["2.8","High",8302]
["2.9","Medium",8303]
["2.99","High",8311]
["3.1","High",8312]
["3.2","Very High",8313]
["3.3","High",8314]
["3.4","Low",8294]
["3.5","Medium",8315]
["3.6","High",8316]
["3.7","Very High",8317]
["3.8","Very High",8318]
["3.99","High",8319]
["4.1","High",8320]
["4.10","High",8329]
["4.11","Medium",8330]
["4.12","Very High",8331]
["4.13","Very High",8332]
["4.14","Very High",8333]
["4.15","Very High",8334]
["4.16","Very High",8335]
["4.17","Very High",8336]
["4.18","Very High",8337]
["4.19","Low",8338]
["4.2","Medium",8321]
["4.20","Very High",8339]
["4.21","High",8340]
["4.22","Low",8341]
["4.23","High",8342]
["4.24","High",8343]
["4.25","Low",8344]
["4.26","Low",8345]
["4.27","High",8346]
["4.3","Medium",8322]
["4.4","High",8323]
["4.5","Very High",8324]
["4.6","Medium",8325]
["4.7","High",8326]
["4.8","Medium",8327]
["4.9","Medium",8328]
["4.99","High",8347]
["5.1","Very High",8517]
["5.10","High",8526]
["5.11","Low",8527]
["5.12","Medium",8528]
["5.13","High",8529]
["5.14","Very High",8530]
["5.15","Medium",8531]
["5.16","Very High",8532]
["5.17","Very High",8533]
["5.18","High",8534]
["5.19","Medium",8535]
["5.2","Very High",8518]
["5.20","Medium",8536]
["5.21","Medium",8537]
["5.22","High",8539]
["5.23","Very High",8540]
["5.24","Very High",8541]
["5.25","Medium",8542]
["5.26","Medium",8543]
["5.27","Medium",8544]
["5.28","Very High",8545]
["5.29","High",8546]
["5.3","Low",8519]
["5.30","High",8547]
["5.31","High",8548]
["5.32","High",8549]
["5.33","High",8550]
["5.34","Low",8551]
["5.35","Medium",8552]
["5.36","Low",8553]
["5.37","Low",8554]
["5.38","High",8555]
["5.39","Very High",8556]
["5.4","High",8520]
["5.40","Very High",8557]
["5.41","Very High",8558]
["5.42","Medium",8559]
["5.43","High",8560]
["5.44","High",8561]
["5.45","Medium",8564]
["5.46","Medium",8565]
["5.47","Medium",8566]
["5.48","Medium",8567]
["5.5","Low",8521]
["5.6","Low",8522]
["5.7","Medium",8523]
["5.8","Medium",8524]
["5.9","Very High",8525]
["5.99","High",8568]
["6.1","Medium",8348]
["6.10","Low",8357]
["6.11","High",8358]
["6.12","Medium",8359]
["6.13","Low",8360]
["6.14","High",8361]
["6.15","High",8362]
["6.16","Very High",8363]
["6.17","Very High",8364]
["6.18","Medium",8365]
["6.19","Low",8366]
["6.2","High",8349]
["6.20","Medium",8367]
["6.21","High",8368]
["6.22","Medium",8369]
["6.3","Low",8350]
["6.4","High",8351]
["6.5","Medium",8352]
["6.6","Medium",8353]
["6.7","High",8354]
["6.8","High",8355]
["6.9","Low",8356]
["6.99","High",8370]
["7.1","High",8371]
["7.10","High",8380]
["7.11","High",8381]
["7.12","High",8382]
["7.13","Medium",8383]
["7.14","Medium",8384]
["7.15","High",8385]
["7.16","High",8386]
["7.17","High",8387]
["7.2","High",8372]
["7.3","Low",8373]
["7.4","Low",8374]
["7.5","Low",8375]
["7.6","Medium",8376]
["7.7","Low",8377]
["7.8","High",8378]
["7.9","High",8379]
["7.99","High",8388]
["8.1","Very High",8569]
["8.10","Very High",8578]
["8.100","Low",11227]
["8.101","Medium",11228]
["8.102","Low",11229]
["8.103","Low",11230]
["8.104","Low",11231]
["8.105","Medium",11232]
["8.106","Medium",11233]
["8.107","Low",11234]
["8.108","High",11235]
["8.109","Very High",11236]
["8.11","Medium",8579]
["8.110","High",11237]
["8.111","Medium",11238]
["8.112","High",11239]
["8.113","Medium",11240]
["8.114","Low",11241]
["8.115","High",11242]
["8.116","Medium",11243]
["8.117","Medium",11244]
["8.118","Medium",11245]
["8.119","High",11246]
["8.12","Medium",8580]
["8.120","High",11247]
["8.121","Medium",11248]
["8.122","High",11249]
["8.123","High",11250]
["8.124","Low",11251]
["8.125","High",11252]
["8.126","Medium",11253]
["8.127","Medium",11254]
["8.13","Medium",8581]
["8.14","Very High",8582]
["8.15","High",8583]
["8.16","Very High",8584]
["8.17","Low",8585]
["8.18","High",8586]
["8.19","High",8587]
["8.199","High",11255]
["8.2","Medium",8570]
["8.20","Medium",8588]
["8.21","High",8589]
["8.22","Very High",8590]
["8.23","Medium",8591]
["8.24","Medium",8592]
["8.25","Very High",8593]
["8.26","High",8594]
["8.27","Medium",8595]
["8.28","Medium",8596]
["8.29","High",8598]
["8.3","Very High",8571]
["8.30","High",8599]
["8.31","High",8600]
["8.32","Low",8601]
["8.33","Medium",8602]
["8.34","High",8603]
["8.35","Medium",8604]
["8.36","Medium",8605]
["8.37","High",8607]
["8.38","Medium",8608]
["8.39","Medium",8609]
["8.4","Medium",8572]
["8.40","High",8610]
["8.41","Medium",8611]
["8.42","Medium",8612]
["8.43","Very High",8613]
["8.44","High",8615]
["8.45","High",8616]
["8.46","Very High",8617]
["8.47","Very High",8618]
["8.48","Medium",8619]
["8.49","High",8620]
["8.5","Very High",8573]
["8.50","Medium",8621]
["8.51","Low",8622]
["8.52","Low",8623]
["8.53","Low",8624]
["8.54","High",8625]
["8.55","Low",11182]
["8.56","Medium",11183]
["8.57","Medium",11184]
["8.58","High",11185]
["8.59","High",11186]
["8.6","Medium",8574]
["8.60","High",11187]
["8.61","Medium",11188]
["8.62","Very High",11189]
["8.63","High",11190]
["8.64","Medium",11191]
["8.65","Low",11192]
["8.66","High",11193]
["8.67","High",11194]
["8.68","High",11195]
["8.69","Medium",11196]
["8.7","High",8575]
["8.70","Medium",11197]
["8.71","Very High",11198]
["8.72","Medium",11199]
["8.73","Medium",11200]
["8.74","High",11201]
["8.75","Medium",11202]
["8.76","Medium",11203]
["8.77","Medium",11204]
["8.78","Medium",11205]
["8.79","Medium",11206]
["8.8","Medium",8576]
["8.80","Medium",11207]
["8.81","Low",11208]
["8.82","Medium",11209]
["8.83","Low",11210]
["8.84","Low",11211]
["8.85","Medium",11212]
["8.86","Medium",11213]
["8.87","Medium",11214]
["8.88","Low",11215]
["8.89","High",11216]
["8.9","High",8577]
["8.90","High",11217]
["8.91","High",11218]
["8.92","Medium",11219]
["8.93","Low",11220]
["8.94","Low",11221]
["8.95","Medium",11222]
["8.96","Medium",11223]
["8.97","Low",11224]
["8.98","High",11225]
["8.99","Medium",11226]
["9.1","Low",8390]
["9.10","Medium",8399]
["9.11","Medium",8400]
["9.12","Medium",8401]
["9.13","Low",8402]
["9.14","Medium",8403]
["9.15","Medium",8404]
["9.16","High",8405]
["9.17","High",8406]
["9.18","Low",8407]
["9.19","Low",8408]
["9.2","Very High",8391]
["9.20","Medium",8409]
["9.21","Medium",8410]
["9.22","Low",8411]
["9.23","Low",8412]
["9.24","Medium",8413]
["9.25","Low",8414]
["9.26","Low",8415]
["9.27","Low",8416]
["9.28","Medium",8417]
["9.29","Low",8418]
["9.3","Very High",8392]
["9.4","High",8393]
["9.5","High",8394]
["9.6","Low",8395]
["9.7","Medium",8396]
["9.8","Medium",8397]
["9.9","Medium",8398]
["9.99","High",8419]

{"sheet":"Equipment_list","index":7,"n_rows":28,"n_cols":3,"rows_kept":28,"cut":false,"hidden":true,"merged":[]}
["TITLE","Equipment_list_description","ID"]
["Accommodation",null,12]
["Cargo Mach.",null,13]
["Critical Equip.",null,16]
["Deck - Machinery",null,18]
["Deck - Mooring Machinery",null,15]
["Deck - Pipe / Fittings",null,20]
["Documentation",null,21]
["E/R - Air Comp.",null,8]
["E/R - Aux. Engine",null,4]
["E/R - Aux. Mach.",null,7]
["E/R - Boiler",null,5]
["E/R - Main Engine",null,3]
["E/R - Pipes/ valves & fittings",null,9]
["E/R - Pumps",null,32]
["E/R - Purifier",null,6]
["Elect. Mach. & Equip.",null,10]
["Hull & Tanks",null,19]
["Inert Gas",null,14]
["LSA / FFA",null,17]
["Miscellaneous",null,22]
["Navigation - DGPS / EPFS / AIS",null,28]
["Navigation - ECDIS",null,25]
["Navigation - Echo Sounder / Speed Log",null,26]
["Navigation - GMDSS & Communication",null,23]
["Navigation - Others",null,11]
["Navigation - RADAR",null,24]
["Navigation - VDR / BNWAS",null,30]

{"sheet":"PSC_MOU","index":8,"n_rows":11,"n_cols":3,"rows_kept":11,"cut":false,"hidden":true,"merged":[]}
["TITLE","PSC_MOU_description","ID"]
["Asia and the Pacific",null,2]
["Caribbean",null,4]
["Europe and the North Atlantic",null,1]
["Latin America",null,3]
["The Black Sea region",null,6]
["The Indian Ocean",null,8]
["The Mediterranean",null,7]
["The Riyadh MoU",null,9]
["USCG",null,10]
["West and Central Africa",null,5]

{"sheet":"Inspection_type","index":9,"n_rows":13,"n_cols":2,"rows_kept":13,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Bunkering Audit",14]
["Cargo Audit",17]
["Engineering Audit",16]
["ISM Audit",2]
["ISPS Audit",3]
["IT Audit",10]
["MLC Audit",1]
["Mooring Audit",9]
["Nav Audit / Verification",8]
["Onboard Training",18]
["Ship Staff Insp.",15]
["Suptd. Insp.",13]

{"sheet":"Deficiency_Cause","index":10,"n_rows":8,"n_cols":3,"rows_kept":8,"cut":false,"hidden":true,"merged":[]}
["TITLE","Deficiency_Cause_description","ID"]
["Behaviour Based",null,1]
["Equipment Related",null,4]
["External Factors",null,5]
["Human Error",null,7]
["Inappropriate Procedure",null,8]
["Industry Issue",null,6]
["Knowledge Based",null,3]

{"sheet":"Observer_code","index":11,"n_rows":3,"n_cols":3,"rows_kept":3,"cut":false,"hidden":true,"merged":[]}
["TITLE","Observer_code_description","ID"]
["Owner / Marine / Tech. Suptd.",null,3]
["Ship Staff",null,2]

{"sheet":"Status_code","index":12,"n_rows":6,"n_cols":3,"rows_kept":6,"cut":false,"hidden":true,"merged":[]}
["TITLE","Status_code_description","ID"]
["Completed",null,6]
["Deferred to D D",null,5]
["In progress",null,3]
["Not Started",null,2]
["Waiting spare",null,4]

{"sheet":"PSC_ref_no","index":13,"n_rows":19,"n_cols":2,"rows_kept":19,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Alarms",9]
["Cargo operations including equipment",7]
["Certificates & Documentation",2]
["Dangerous Goods",13]
["Emergency Systems",5]
["Fire safety",8]
["ISM",16]
["ISPS",17]
["Life saving appliances",12]
["MLC, 2006",18]
["Other",19]
["Pollution Prevention",15]
["Propulsion and auxiliary machinery",14]
["Radio communication",6]
["Safety of Navigation",11]
["Structural condition",3]
["Water/Weathertight condition",4]
["Working and Living Conditions",10]

{"sheet":"Risk_value_of_obs","index":14,"n_rows":1,"n_cols":2,"rows_kept":1,"cut":false,"hidden":true,"merged":[]}
["Risk Value of observation","ID"]

{"sheet":"Year","index":15,"n_rows":18,"n_cols":1,"rows_kept":18,"cut":false,"hidden":true,"merged":[]}
["Year"]
[2014]
[2015]
[2016]
[2017]
[2018]
[2019]
[2020]
[2021]
[2022]
[2023]
[2024]
[2025]
[2026]
[2027]
[2028]
[2029]
[2030]

{"sheet":"Month","index":16,"n_rows":13,"n_cols":1,"rows_kept":13,"cut":false,"hidden":true,"merged":[]}
["Month"]
["Jan"]
["Feb"]
["Mar"]
["Apr"]
["May"]
["Jun"]
["Jul"]
["Aug"]
["Sep"]
["Oct"]
["Nov"]
["Dec"]

{"sheet":"Date_","index":17,"n_rows":32,"n_cols":1,"rows_kept":32,"cut":false,"hidden":true,"merged":[]}
["Date"]
["01"]
["02"]
["03"]
["04"]
["05"]
["06"]
["07"]
["08"]
["09"]
[10]
[11]
[12]
[13]
[14]
[15]
[16]
[17]
[18]
[19]
[20]
[21]
[22]
[23]
[24]
[25]
[26]
[27]
[28]
[29]
[30]
[31]

{"sheet":"Sheet1","index":18,"n_rows":24,"n_cols":6,"rows_kept":24,"cut":false,"hidden":true,"merged":[]}
[]
[null,"ID","E",null,"Date Recorded",1]
[null,"UNIQUE ID","F",null,"Type of Deficiency",2]
[1,"Date Recorded","G",null,"Observer code",3]
["ignore","Vessel Type","H",null,"Type of Inspection",4]
[null,"Internal / External","I",null,"Description of Deficiency",5]
[null,"Drydock","J",null,"Equipment Categories",6]
[null,"Information Sharing","K",null,"Area of Observation",7]
[null,"Critical_item","L",null,"Deficiency Cause",8]
[null,"Deficiency Type","M",null,"VIQ Ref Number",9]
[null,"Deficiency Cause","N",null,"Risk Value of Obs",10]
[null,"Inspection Type","O",null,"PSC Ref Number",11]
[null,"Equipments","P",null,"PSC MOU ID",12]
[null,"VIQ Reference Number","Q",null,"Action Taken or Required",13]
[null,"Risk Value of the observation","R",null,"Target Date",14]
[null,"PSC Reference Number","S",null,"PO Ref No.",15]
[null,"PSC MOU","T",null,"Status Code",16]
[null,"Observer Code","U",null,"Date Completed",17]
[null,"Target Date","V",null,"Drydock",18]
[null,"Status Code","W",null,"Info Sharing",19]
[null,"Description of Deficiency","X",null,"Critical Item Flag",20]
[null,"Action taken / required","Y",null,"Audit Type",21]
[null,"PO ref no","Z"]
[null,"Date completed","AA"]

{"sheet":"Ship_information","index":19,"n_rows":2,"n_cols":3,"rows_kept":2,"cut":false,"hidden":true,"merged":[]}
["Ship_ID","Ship_Name","FILE_NAME"]
["57","DHT STALLION (31-05-2023)","57_1685525919619.xlsm"]

{"sheet":"External_Deficiency_type","index":20,"n_rows":5,"n_cols":3,"rows_kept":5,"cut":false,"hidden":true,"merged":[]}
["TITLE","Type of deficiency_description","ID"]
["Condn of Class / Memo",null,5]
["Defect",null,1]
["Non Conformity",null,2]
["Observation",null,3]

{"sheet":"External_Inspection_type","index":21,"n_rows":11,"n_cols":2,"rows_kept":11,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Cargo Audit",17]
["Flag State Insp.",5]
["ISM Audit",2]
["ISPS Audit",3]
["MLC Audit",1]
["Nav Audit / Verification",8]
["OM Insp. (Eg. SIRE / CDI etc.)",6]
["Others (Eg. Insurance etc.)",12]
["PSC Inspection",4]
["Terminal Insp.",11]

{"sheet":"External_Observer_code","index":22,"n_rows":7,"n_cols":3,"rows_kept":7,"cut":false,"hidden":true,"merged":[]}
["TITLE","Observer_code_description","ID"]
["Class Surveyor",null,4]
["FSC Inspector",null,5]
["Others (Eg. Insurance etc.)",null,9]
["PSC Insp.",null,6]
["SIRE / CDI Insp.",null,8]
["Terminal Insp.",null,7]

{"sheet":"Sheet Version","index":23,"n_rows":2,"n_cols":2,"rows_kept":2,"cut":false,"hidden":true,"merged":[]}
["Version","Title"]
["2.0","Version 2.0"]