{"text_format":"1","workbook":"xlsx","n_sheets":24,"sheets":["Mainsheet","Completed","Calc","Areaofobs","Vessel_type","Deficiency_type","VIQrefno","Equipment_list","PSC_MOU","Inspection_type","Deficiency_Cause","Observer_code","Status_code","PSC_ref_no","Risk_value_of_obs","Year","Month","Date_","Sheet1","Ship_information","External_Deficiency_type","External_Inspection_type","External_Observer_code","Sheet Version"],"not_rendered":{"charts":0,"images":1,"macros":1,"external_links":0,"defined_names":12,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Mainsheet","index":0,"n_rows":22,"n_cols":28,"rows_kept":22,"cut":false,"hidden":false,"merged":[[10,8,10,9],[10,12,10,13],[12,6,12,27],[8,6,8,27]]}
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,"Defect - Damage Monitoring Sheet"]
[]
[null,null,null,null,null,null,null,"Date of Report","21-Aug-2023",null,null,"Ship Name","AQUAHOLIC (19-12-2022)"]
[]
[null,null,null,null,null,null,"VERSION : 2.0"]
[]
[]
[]
[null,null,null,"ID","SHIPSIDE UNIQUEID","UNIQUE ID","Date Recorded","Type of Deficiency","Observer code","Type of Inspection","Description of Deficiency","Equipment Categories","Area of Observation","Deficiency Cause","VIQ Ref Number","Risk Value of Obs","PSC Ref Number","PSC MOU ID","Action Taken or Required","Target Date","PO Ref No.","Status Code","Date Completed","Drydock","Info Sharing","Critical Item","Audit Type","Superintendent Remarks"]
[null,null,null,null,25575,"0_Thu Nov 17 2022 16:48:58 GMT+0800","2022-09-24T08:00:00","Critical Equipment,Breakdown,Defect,Observation","Ship Staff","Ship Staff Insp.","Fore peak tank Electro Hyd valve not operational from Remote station(Bridge).","Hull & Tanks","Cargo / Ballast Systems","Equipment Related","","","","","Need to renew the operating unit and try out from Remote & local stations. Awaiting spares.","2023-08-30T08:00:00","NAQU220148 is partially received, only manual operating handle is received.","Waiting spare",null,"No","No","No","Internal","RO is under processing , waiting approval from owner, will inspect at shipyard and manage to rectify."]
[null,null,null,null,16899,"122_Mon Feb 27 2023 13:45:16 GMT+0800","2023-02-16T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Provision Exhaust fan motor not operational. ","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","New motor to install. Awaiting spares. ","2023-08-30T08:00:00","NAQU230064","Waiting spare",null,"No","No","No","Internal","RO is under processing will connect to vessel once ready"]
[null,null,null,null,78451,"122_Wed Aug 16 2023 00:50:36 GMT+0800","2023-08-15T08:00:00","Observation","Ship Staff","Ship Staff Insp.","Fresh water pipe on-deck corroded and water leaking .","Deck - Pipe / Fittings","General Appearance","External Factors","","","","","Pipe has to be renew.","2023-08-30T08:00:00","","In progress",null,"No","No","No","Internal"]
[null,null,null,null,45783,"122_Mon Aug 21 2023 15:14:35 GMT+0800","2023-08-21T08:00:00","Defect","Ship Staff","Ship Staff Insp.","The casing is corroded / worn out beyond repairs in way of  mouth rings and stage rings. Pressure is lower than normal. No.1 pump can be used in boiler low pressure. Requisition has been raised.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","","","","","WAITING SPARE.","2023-08-31T08:00:00","NAQU230251 - BOILER FEED WATER PUMP NO.1","Waiting spare",null,"No","No","No","Internal"]
[null,null,null,null,23685,"122_Mon Aug 21 2023 18:41:56 GMT+0800","2023-08-21T08:00:00","Defect","Ship Staff","Ship Staff Insp.","FISH ROOM AUTO DEFROST TIMER IS DEFECTIVE. REQUISITION HAS BEEN RAISED.","Elect. Mach. & Equip.","MLC Related","Equipment Related","","","","","FISH ROOM DEFROSTING IS CARRYING OUT MANUALLY ON REGULAR INTERVAL.","2023-08-31T08:00:00","NAQU230278 - AUTO DEFROST TIMER - REF. PROV. PLANT - ELECTRIC","Waiting spare",null,"No","No","No","Internal"]

{"sheet":"Completed","index":1,"n_rows":227,"n_cols":28,"rows_kept":227,"cut":false,"hidden":false,"merged":[[10,8,10,9],[10,12,10,13],[12,6,12,27],[8,6,8,27]]}
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,"Defect - Damage Monitoring Sheet"]
[]
[null,null,null,null,null,null,null,"Date of Report","21-Aug-2023",null,null,"Ship Name","AQUAHOLIC (19-12-2022)"]
[]
[null,null,null,null,null,null,"VERSION : 2.0"]
[]
[]
[]
[null,null,null,"ID","SHIPSIDE UNIQUEID","UNIQUE ID","Date Recorded","Type of Deficiency","Observer code","Type of Inspection","Description of Deficiency","Equipment Categories","Area of Observation","Deficiency Cause","VIQ Ref Number","Risk Value of Obs","PSC Ref Number","PSC MOU ID","Action Taken or Required","Target Date","PO Ref No.","Status Code","Date Completed","Drydock","Info Sharing","Critical Item","Audit Type","Superintendent Remarks"]
[null,null,null,25685,null,"122_14/6/2022 10:33:21 pm","2021-04-19T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Emergency Stop peddle on bench grinder and bench drill should be secured properly to the floor. ","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","Emergency stop peddle switch secured and area marked, crew briefed about the usage.","2022-05-19T23:59:35","","Completed","2022-05-02T23:59:35","No","No","No","Internal"]
[null,null,null,21125,null,"122_17-09-2021 08:46:05","2021-07-30T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Galley oven is rusty from inside.","Accommodation,LSA / FFA,Miscellaneous","MLC Related","Equipment Related","","","","","De-rusting and removed the rust insidegalley oven. Tray cleanedand oven inside plating wirebrushed.","2021-10-29T23:59:35","","Completed","2021-09-17T23:59:35","No","No","No","Internal"]
[null,null,null,21126,null,"122_17-09-2021 09:21:51","2021-07-30T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Flour mixer in galley is defective. ","Accommodation","MLC Related","Equipment Related","","","","","The blade for the flour mixer was adjusted and rectified","2021-10-29T23:59:35","","Completed","2021-09-17T23:59:35","No","No","No","Internal"]
[null,null,null,21179,null,"122_17-09-2021 08:20:03","2021-07-30T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Crew messroom doesnot have microwave oven.","Accommodation,Miscellaneous","MLC Related","Equipment Related","","","","","Requsition raised for new microwave.","2021-10-29T23:59:35","","Completed","2021-08-17T23:59:35","No","No","No","Internal"]
[null,null,null,21188,null,"122_16-09-2021 06:50:50","2021-07-30T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Main engine Main starting air valve is operating tight,also limit switch for the open condition indicator is loose","E/R - Main Engine,Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","Limit Switch tightened,Valave to check","2021-08-30T23:59:35","","Completed","2021-07-30T23:59:35","No","No","No","Internal"]
[null,null,null,21123,null,"122_30/8/2021 1:44:07 am","2021-07-31T23:59:35","Defect","Ship Staff","Ship Staff Insp.","NO.5 cargo hold water ingress system pre-alarm inoperational.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","","","","","Received PO. NAQU210051 spare WIAS sensor. Vessel repaired the present sensor while at discharge port.","2022-02-15T23:59:35","NAQU210051","Completed","2022-01-21T23:59:35","No","No","No","Internal","spare sensor connected to vessel already. pls check and revert."]
[null,null,null,21130,null,"122_31/8/2021 12:00:19 am","2021-07-31T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Echo Sounder printer stylus is broken, need new spare. Meantime vessel is trying to locate if any spares available.","Navigation - Echo Sounder / Speed Log","Navigation","Equipment Related","","","","","Stylus replaced with new spare received at singapore","2021-10-30T23:59:35","","Completed","2021-09-15T23:59:35","No","No","No","Internal"]
[null,null,null,21180,null,"122_30/8/2021 11:39:45 pm","2021-07-31T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Speed log showing erratic reading","Navigation - Echo Sounder / Speed Log","Navigation","Equipment Related","","","","","Speed log shore trouble shooting carried out as per office advice and fault rectified. Performance is being monitored.","2021-10-30T23:59:35","","Completed","2021-08-10T23:59:35","No","No","No","Internal"]
[null,null,null,21181,null,"122_31/8/2021 8:15:12 pm","2021-07-31T23:59:35","Defect","Ship Staff","Ship Staff Insp.","All the mooring winches require greasing.","Deck - Mooring Machinery","Mooring","Equipment Related","","","","","All mooring winches greased.","2021-08-26T23:59:35","","Completed","2021-08-03T23:59:35","No","No","No","Internal"]
[null,null,null,21182,null,"122_31/8/2021 8:20:46 pm","2021-07-31T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Guide wire for hatches no.1 & no.3 require greasing.","Deck - Machinery","Structural Condn. / WT integrity ","Equipment Related","","","","","Greasing of guide wire carried out.","2021-08-26T23:59:35","","Completed","2021-08-09T23:59:35","No","No","No","Internal"]
[null,null,null,21183,null,"122_16-09-2021 06:32:01","2021-07-31T23:59:35","Defect","Ship Staff","Ship Staff Insp.","No.2 fire ,bilge &GS  pump Water Leaking from gland","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","","","","","Top two gland packing renewed.To check condition of shaft and sleeve","2021-09-10T23:59:35","","Completed","2021-08-21T23:59:35","No","No","No","Internal"]
[null,null,null,21122,null,"122_31/8/2021 12:12:03 am","2021-08-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Hatch cover hydraulic pipelines on main deck for most of the holds are in poor condition and thinned down especially at the U-clamp areas.","Deck - Pipe / Fittings","ISM Related","Equipment Related","","","","","REPETETIVE ENTRY","2021-10-30T23:59:35","","Completed","2021-09-25T23:59:35","No","No","No","Internal"]
[null,null,null,21132,null,"122_31/8/2021 12:16:24 am","2021-08-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","No.2 hatch operating lever block having a leak, suspect it is from the emergency connection.","Deck - Pipe / Fittings","ISM Related","Equipment Related","","","","","Emergency connection removed and gasket replaced and leak rectified","2021-10-31T23:59:35","","Completed","2021-09-17T23:59:35","No","No","No","Internal"]
[null,null,null,21133,null,"122_31/8/2021 12:20:00 am","2021-08-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Most of the hatch cover natural vents rubber packings need replacement.","Hull & Tanks","Structural Condn. / WT integrity ","Equipment Related","","","","","Renewed all damaged natural vents rubber packing.","2021-10-31T23:59:35","","Completed","2021-09-01T23:59:35","No","No","No","Internal"]
[null,null,null,21137,null,"122_30/8/2021 11:24:37 pm","2021-08-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Few of the cargo hold booby hatch cover packing require renewal","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","External Factors,Inappropriate Procedure","","","","","Rubber packing for booby hatches of CH. 7 & 3 renewed.","2021-10-31T23:59:35","","Completed","2021-09-01T23:59:35","No","No","No","Internal"]
[null,null,null,21138,null,"122_31/8/2021 11:23:12 am","2021-08-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Deck standing mooring rollers are frozen","Deck - Pipe / Fittings","Mooring","External Factors,Inappropriate Procedure","","","","","Deck Standing Mooring rollers for fwd and aft spring lines freed up and operational.","2021-11-01T23:59:35","","Completed","2021-10-09T23:59:35","No","No","No","Internal"]
[null,null,null,21139,null,"122_31/8/2021 11:25:21 am","2021-08-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Accommodation ladder lower platform roller is frozen.","Deck - Pipe / Fittings","General Appearance","Equipment Related,Inappropriate Procedure","","","","","Lower platform rollers to be freed up","2021-09-30T23:59:35","","Completed","2021-09-24T23:59:35","No","No","No","Internal"]
[null,null,null,21140,null,"122_17-09-2021 07:16:16","2021-08-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Vessel has only 1 de-mucking winch motor operational, need spares and additional motor to speed up hatch cleaning.","Cargo Mach.","General Appearance","Equipment Related","","","","","damaged de mucking winch repaired.","2021-10-28T23:59:35","","Completed","2021-09-11T23:59:35","No","No","No","Internal"]
[null,null,null,21184,null,"122_31/8/2021 12:22:06 pm","2021-08-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Stbd provision crane swivel needs freeing up","Deck - Pipe / Fittings","General Appearance","Inappropriate Procedure","","","","","Provision crane swivel freeing and greasing carried out","2021-09-30T23:59:35","","Completed","2021-08-09T23:59:35","No","No","No","Internal"]
[null,null,null,21185,null,"122_31/8/2021 5:14:15 pm","2021-08-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Hatch cover opening guide wheels/ sheaves / chain sprockets require greasing.","Deck - Pipe / Fittings","General Appearance","External Factors,Inappropriate Procedure","","","","","Hatch cover opening guide wheels/ sheaves and chain sprockets greasing carried out.","2021-11-01T23:59:35","","Completed","2021-08-13T23:59:35","No","No","No","Internal"]
[null,null,null,21186,null,"122_16-09-2021 06:40:19","2021-08-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","No.1 fire and Bilge & GS pump water leaking from gland.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","","","","","Top Gland packings renewed.","2021-09-01T23:59:35","","Completed","2021-08-12T23:59:35","No","No","No","Internal"]
[null,null,null,21141,null,"122_31/8/2021 6:15:44 pm","2021-08-02T23:59:35","Defect","Ship Staff","Ship Staff Insp.","No.1 cargo hold wheel lifter found leaking when in operation.","Deck - Machinery","ISM Related","Equipment Related","","","","","adapter on lift cylinder removed and oring changed.","2021-11-01T23:59:35","","Completed","2021-09-23T23:59:35","No","No","No","Internal"]
[null,null,null,21143,null,"122_31/8/2021 6:23:00 pm","2021-08-02T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Wheel lifter isolation valves for all hatch covers seems frozen.","Deck - Machinery","ISM Related","Equipment Related","","","","","FLow control valves were eased up and rectified.","2021-11-01T23:59:35","","Completed","2021-09-19T23:59:35","No","No","No","Internal"]
[null,null,null,21146,null,"122_31/8/2021 7:28:32 pm","2021-08-02T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Rescue boat davit accummalator charging valve wheel needs to be replaced.","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","damaged valve wheel replaced with new spare wheel.","2021-11-01T23:59:35","","Completed","2021-09-10T23:59:35","No","No","No","Internal"]
[null,null,null,21150,null,"122_17-09-2021 08:54:52","2021-08-02T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Ship's laundry wash basin drain is choked.","Accommodation","MLC Related","Equipment Related","","","","","Drain choke was cleared","2021-11-01T23:59:35","","Completed","2021-09-25T23:59:35","No","No","No","Internal"]
[null,null,null,21178,null,"122_30/8/2021 1:46:36 am","2021-08-02T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Helicopter Operations Fireman's suit condition has deteriorated and needs to be replaced.","LSA / FFA","Safety / LSA / FFA","Human Error,Inappropriate Procedure","","","","","Spare fireman outfit ordered and replaced defective suit.","2021-09-01T23:59:35","NAQU210013","Completed","2021-08-22T23:59:35","No","No","No","Internal"]
[null,null,null,21187,null,"122_31/8/2021 6:32:08 pm","2021-08-02T23:59:35","Defect","Ship Staff","Ship Staff Insp.","few of the hatch cover cleats nuts needs freeing up.","Deck - Machinery","ISM Related","Equipment Related","","","","","All cleats freed up and greased.","2021-08-15T23:59:35","","Completed","2021-08-13T23:59:35","No","No","No","Internal"]
[null,null,null,21189,null,"122_16-09-2021 07:04:23","2021-08-02T23:59:35","Defect","Ship Staff","Ship Staff Insp.","ME No.4 Unit steam smoothering connection found leaking","E/R - Main Engine,E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Leakage to be rectified","2021-09-05T23:59:35","","Completed","2021-08-05T23:59:35","No","No","No","Internal"]
[null,null,null,21151,null,"122_17-09-2021 07:30:02","2021-08-03T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Keep chain in many locations are rusted, require derusting and painting.","Deck - Pipe / Fittings","General Appearance","Equipment Related","","","","","REPETITIVE ENTRY","2021-11-02T23:59:35","","Completed","2021-09-25T23:59:35","No","No","No","Internal"]
[null,null,null,21152,null,"122_31/8/2021 8:12:45 pm","2021-08-03T23:59:35","Defect","Ship Staff","Ship Staff Insp.","At many locations F-keys are not available near to valves on deck","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","new F-keys fabricated and placed near the valves","2021-11-02T23:59:35","","Completed","2021-09-08T23:59:35","No","No","No","Internal"]
[null,null,null,21155,null,"122_31/8/2021 8:02:19 pm","2021-08-03T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Few of the walkie talkies are in poor condition and few of them are with very poor reception & sound.","Navigation - GMDSS & Communication","Safety / LSA / FFA","Equipment Related","","","","","Spares received onboard and defective parts replaced.","2021-11-02T23:59:35","","Completed","2021-09-20T23:59:35","No","No","No","Internal"]
[null,null,null,21157,null,"122_31/8/2021 9:13:51 pm","2021-08-03T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Keep chains in many locations are rusted, require derusting and painting","Deck - Pipe / Fittings","General Appearance","External Factors,Inappropriate Procedure","","","","","All safety keep chain derusted and painted.","2021-11-25T23:59:35","","Completed","2021-11-15T23:59:35","No","No","No","Internal","pls update status."]
[null,null,null,21160,null,"122_9/18/2021 12:56:44 PM","2021-08-03T23:59:35","Defect","Ship Staff","Ship Staff Insp.","The garbage bins in common spaces are in poor condition.","Accommodation,Miscellaneous","General Appearance","Human Error,Inappropriate Procedure","","","","","All common places garbage bins replaced with new ones.","2021-11-06T23:59:35","","Completed","2021-09-22T23:59:35","No","No","No","Internal"]
[null,null,null,21161,null,"122_9/18/2021 1:01:43 PM","2021-08-03T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Mooring ropes are stained with cargo deposit and have abrasion damage / rope degradation. Need to have a close up inspection for the same.","Deck - Mooring Machinery","ISM Related","Inappropriate Procedure","","","","","Lay out all mooring ropes on deck and wash it using high pressure washing machine to remove the cargo residues. Then carry out close up inspection.","2021-11-03T23:59:35","","Completed","2021-09-05T23:59:35","No","No","No","Internal"]
[null,null,null,21190,null,"122_9/18/2021 12:54:17 PM","2021-08-03T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Most of the galley cooking utensils base need to buff clear off burnt deposits.","Accommodation,Miscellaneous","General Appearance","Equipment Related,Inappropriate Procedure","","","","","All galley utensils buffed and cleaned the base. Clear of all burnt marks and deposits.","2021-11-02T23:59:35","","Completed","2021-09-08T23:59:35","No","No","No","Internal"]
[null,null,null,21191,null,"122_9/18/2021 8:23:20 AM","2021-08-03T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Provision room lobby entrance door handle is defective.","Accommodation,Deck - Pipe / Fittings","Structural Condn. / WT integrity ","Equipment Related,Inappropriate Procedure","","","","","Repair the weathertight door dogs and lubricate.","2021-11-06T23:59:35","","Completed","2021-08-15T23:59:35","No","No","No","Internal"]
[null,null,null,21192,null,"122_9/18/2021 7:24:26 AM","2021-08-03T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Provision room lobby flooring is rusted.","Accommodation,Miscellaneous","General Appearance","External Factors,Inappropriate Procedure","","","","","Carry out de-rusting and paint it.","2021-10-25T23:59:35","","Completed","2021-08-14T23:59:35","No","No","No","Internal"]
[null,null,null,21193,null,"122_9/18/2021 7:20:22 AM","2021-08-03T23:59:35","Defect","Ship Staff","Ship Staff Insp.","One of the galley drain was found choked.","Accommodation,Deck - Pipe / Fittings","MLC Related","Human Error,Inappropriate Procedure","","","","","Cleared the debris from the choked drain pipe.","2021-11-02T23:59:35","","Completed","2021-08-05T23:59:35","No","No","No","Internal"]
[null,null,null,21194,null,"122_9/18/2021 6:53:34 AM","2021-08-03T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Faucet in galley & Officer pantry found leaking.","Accommodation,Deck - Pipe / Fittings","General Appearance","Equipment Related","","","","","Repair the leaking faucet / tap.","2021-11-02T23:59:35","","Completed","2021-09-11T23:59:35","No","No","No","Internal"]
[null,null,null,21195,null,"122_31/8/2021 9:08:07 pm","2021-08-03T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Accommodation ladder and gangway sheaves require greasing / maintenance.","Miscellaneous","General Appearance","Human Error,Inappropriate Procedure","","","","","Greasing of sheaves carried out.","2021-11-02T23:59:35","","Completed","2021-08-11T23:59:35","No","No","No","Internal"]
[null,null,null,21196,null,"122_16-09-2021 06:56:24","2021-08-03T23:59:35","Defect","Ship Staff","Ship Staff Insp.","ME No.1 unit FWD fuel valve found leaking from the body","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Fuel valve to be renewed with overhauled one.","2021-08-04T23:59:35","","Completed","2021-11-03T23:59:35","No","No","No","Internal"]
[null,null,null,21197,null,"122_16-09-2021 07:00:02","2021-08-03T23:59:35","Defect","Ship Staff","Ship Staff Insp.","ME under piston door leaking in way of tightening bolts","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Gaskets to be renewed.","2021-08-04T23:59:35","","Completed","2021-10-03T23:59:35","No","No","No","Internal"]
[null,null,null,21198,null,"122_9/18/2021 12:46:10 PM","2021-08-03T23:59:35","Defect","Ship Staff","Ship Staff Insp.","No music player / system in crew smoke room.","Accommodation,Miscellaneous","MLC Related","Equipment Related","","","","","Raised requsition for music system.","2021-07-06T23:59:35","","Completed","2021-08-17T23:59:35","No","No","No","Internal"]
[null,null,null,21199,null,"122_9/18/2021 10:50:44 AM","2021-08-03T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Two common toilet shower mixers defective.","Accommodation","MLC Related","Equipment Related","","","","","Two nos shower mixer received and defective shower mixers replaced.","2021-09-25T23:59:35","NAQU210056","Completed","2021-08-17T23:59:35","No","No","No","Internal"]
[null,null,null,21200,null,"122_9/18/2021 10:48:07 AM","2021-08-03T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Washing machine and dryer in laundry is defective.\n\n(Only one laundry available for the entire crew, where there is only one machine each for boiler suit, clean clothes and drying, the performance of which is poor. Boiler suit machine does not work if more than one boiler suit is put inside)","Accommodation","MLC Related","Equipment Related","","","","","New washing machine and dryer received and same installed","2021-11-02T23:59:35","","Completed","2021-08-22T23:59:35","No","No","No","Internal"]
[null,null,null,21162,null,"122_17-09-2021 07:06:49","2021-08-04T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Accomodation ladder and gangway sheaves require greasing / maintenance.","Deck - Machinery","ISM Related","Equipment Related,Inappropriate Procedure","","","","","Greasing of both accomodation ladder and gangway carrried out. All sheaves cleaned and applied fresh grease.","2021-11-02T23:59:35","","Completed","2021-09-24T23:59:35","No","No","No","Internal"]
[null,null,null,21201,null,"122_30/8/2021 11:02:57 pm","2021-08-04T23:59:35","Defect","Ship Staff","Ship Staff Insp.","MF/HF ATU found burned","Navigation - GMDSS & Communication","Communication","Equipment Related","","","","","MF/HF ATU replaced with new unit","2021-09-03T23:59:35","","Completed","2021-08-23T23:59:35","No","No","No","Internal"]
[null,null,null,21163,null,"122_16-09-2021 14:00:48","2021-08-05T23:59:35","Defect","Ship Staff","Ship Staff Insp.","No.2 water ballast pump discharge T-Section found welded with doubler plate","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Pipe section to be renewed.","2021-10-05T23:59:35","","Completed","2021-10-16T23:59:35","No","No","No","Internal"]
[null,null,null,21202,null,"122_16-09-2021 07:17:29","2021-08-06T23:59:35","Defect","Ship Staff","Ship Staff Insp.","No.1 Main cooling sea water pump water leaking from gland .","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","","","","","Galnd packing to be renewed.","2021-08-25T23:59:35","","Completed","2021-08-12T23:59:35","No","No","No","Internal"]
[null,null,null,21203,null,"122_16-09-2021 07:21:24","2021-08-06T23:59:35","Defect","Ship Staff","Ship Staff Insp.","No.2 Main cooling sea water pump water leaking from gland","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","","","","","Gland packing to be renewed","2021-08-25T23:59:35","","Completed","2021-08-12T23:59:35","No","No","No","Internal"]
[null,null,null,21204,null,"122_16-09-2021 07:46:19","2021-08-06T23:59:35","Defect","Ship Staff","Ship Staff Insp.","No.1 Ballast Pump water leaking from gland","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","","","","","Gland Packing renewed","2021-08-25T23:59:35","","Completed","2021-08-12T23:59:35","No","No","No","Internal"]
[null,null,null,21205,null,"122_16-09-2021 07:48:42","2021-08-06T23:59:35","Defect","Ship Staff","Ship Staff Insp.","No.2 Ballast Pump water leaking from gland","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","","","","","Gland packings renewed","2021-08-25T23:59:35","","Completed","2021-08-12T23:59:35","No","No","No","Internal"]
[null,null,null,21206,null,"122_16-09-2021 07:25:46","2021-08-09T23:59:35","Defect","Ship Staff","Ship Staff Insp.","HFO transfer pump leaking from gland","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","","","","","Gland packing renewed","2021-09-10T23:59:35","","Completed","2021-08-29T23:59:35","No","No","No","Internal"]
[null,null,null,21207,null,"122_16-09-2021 09:45:01","2021-08-09T23:59:35","Defect","Ship Staff","Ship Staff Insp.","NO.2 Main cooling sea water pump, discharge line elbow found leaking.Found doubler plate welded on elbow section.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Elbow renewed","2021-09-10T23:59:35","","Completed","2021-08-11T23:59:35","No","No","No","Internal"]
[null,null,null,21208,null,"122_17-09-2021 07:25:48","2021-08-09T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Lifeboat flash light found broken.","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","Replaced the broken flashlight with new one.","2021-11-07T23:59:35","","Completed","2021-08-10T23:59:35","No","No","No","Internal"]
[null,null,null,21209,null,"122_16-09-2021 09:28:45","2021-08-11T23:59:35","Defect","Ship Staff","Ship Staff Insp.","AE fresh water cooler No.1 both inlet and outlet fresh water valves found seized in open condition.hence cooler could not be cleaned.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Valves renewed.(Black out job)","2021-09-11T23:59:35","","Completed","2021-08-14T23:59:35","No","No","No","Internal"]
[null,null,null,21168,null,"122_16-09-2021 08:59:12","2021-08-12T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Incinerator Charging door refractory found damaged.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Refractory need to repair","2021-09-25T23:59:35","","Completed","2021-09-16T23:59:35","No","No","No","Internal"]
[null,null,null,21210,null,"122_16-09-2021 14:13:19","2021-08-15T23:59:35","Defect","Ship Staff","Ship Staff Insp.","AE fresh water cooler No.1 sea water outlet pipe section found with pin hole leak.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Pipe section renewed.","2021-09-15T23:59:35","","Completed","2021-09-10T23:59:35","No","No","No","Internal"]
[null,null,null,21170,null,"122_16-09-2021 14:55:54","2021-08-16T23:59:35","Defect","Ship Staff","Ship Staff Insp.","AE LO Purifier No.1 was showing high starting current and not reducing while running.","E/R - Purifier","Eng. / Strg. Comp.","Equipment Related","","","","","LO Purifier No.1 assembled with new spares and working satisfactory.","2021-11-25T23:59:35","","Completed","2021-12-10T23:59:35","No","No","No","Internal","spare will be connected to vessel at next convenient port."]
[null,null,null,21171,null,"122_9/18/2021 1:22:22 PM","2021-08-19T23:59:35","Defect","Ship Staff","Ship Staff Insp.","In cargo hold No. 4 one step missing on the vertical ladder.","Hull & Tanks","ISM Related","Equipment Related,Human Error","","","","","Fabricated missing step on the vertical ladder.","2021-11-18T23:59:35","","Completed","2021-11-01T23:59:35","No","No","No","Internal","pls update status latest."]
[null,null,null,21211,null,"122_16-09-2021 14:23:08","2021-08-24T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","Sewage treatment plant air compressor bearing found damaged.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","STP air compressor bearing renewed","2021-09-25T23:59:35","","Completed","2021-08-25T23:59:35","No","No","No","Internal"]
[null,null,null,21212,null,"122_16-09-2021 14:36:19","2021-08-31T23:59:35","Defect","Ship Staff","Ship Staff Insp.","ME LO cooler Sea water inlet pipe elbow found leaking from welding seam.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Inlet pipe removed and repaired.","2021-09-30T23:59:35","","Completed","2021-09-02T23:59:35","No","No","No","Internal"]
[null,null,null,21915,null,"122_16-10-2021 20:25:53","2021-09-15T23:59:35","Defect","Ship Staff","Ship Staff Insp.","No.1 Fire& GS pump AFT peak line T-Section found with pin hole leak","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Pipe section removed and renewed","2021-10-25T23:59:35","","Completed","2021-09-27T23:59:35","No","No","No","Internal"]
[null,null,null,21916,null,"122_16-10-2021 20:08:16","2021-09-26T23:59:35","Defect","Ship Staff","Ship Staff Insp.","AE jacket cooler(PORT)SW inlet pipe found with pin hole leaks and temporary repair with hose bands.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Pipe section removed and renewed","2021-10-27T23:59:35","","Completed","2021-10-08T23:59:35","No","No","No","Internal"]
[null,null,null,21909,null,"122_16-10-2021 20:19:15","2021-09-28T23:59:35","Defect","Ship Staff","Ship Staff Insp.","AUx cooling SW line to overboard found with pin hole leak at bottom platform","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Pipe section renewed at Norfolk anchorage","2021-12-25T23:59:35","","Completed","2021-11-21T23:59:35","No","No","No","Internal","pls schedule and get it done safely."]
[null,null,null,21917,null,"122_18-10-2021 15:57:04","2021-10-02T23:59:35","Defect","Ship Staff","Ship Staff Insp.","general use handling crane jib sheave was found not rotating when hook was lowered / hoisted without weight.","Deck - Machinery","ISM Related","Equipment Related","","","","","Greasing carried out for sheaves and freed. ","2022-01-01T23:59:35","","Completed","2021-10-05T23:59:35","No","No","No","Internal"]
[null,null,null,21918,null,"122_18-10-2021 16:03:35","2021-10-02T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Stbd anchor cable was found twist when heaved up after Suez anchorage.","Deck - Mooring Machinery","Mooring","Equipment Related","","","","","At next anchorage in Port Said, Egypt the stbd anchor chain twist was removed and cleared.","2022-01-01T23:59:35","","Completed","2021-10-04T23:59:35","No","No","No","Internal"]
[null,null,null,21913,null,"122_16-10-2021 20:11:42","2021-10-08T23:59:35","Defect","Ship Staff","Ship Staff Insp.","AE Jacket cooler(PORT) SW outlet pipe found with doubler welded","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Pipe to be renewed","2021-12-10T23:59:35","","Completed","2021-10-26T23:59:35","No","No","No","Internal"]
[null,null,null,22387,null,"122_31-10-2021 19:31:31","2021-10-16T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Soft patches found on SW pipeline.To rectify at anchorge by permanent repairs(inserts or pipe replacement) as required.  ","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","SW pipe lines with soft patch repair has been removed and permanant repair carried out with new pipe section at Norfolk anchorage","2022-01-05T23:59:35","","Completed","2021-11-27T23:59:35","No","No","No","Internal","pls update latest status."]
[null,null,null,22391,null,"122_31-10-2021 17:35:44","2021-10-16T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ER bilge wells found with sheen of oil,need to clean bilges","Miscellaneous","General Appearance","Equipment Related","","","","","ER Bilge wells emptied and cleaned","2021-10-17T23:59:35","","Completed","2021-10-17T23:59:35","No","No","No","Internal"]
[null,null,null,22392,null,"122_31-10-2021 19:15:17","2021-10-16T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ME Fuel Pump Save Oils & area between cylinders found with oil deposits","E/R - Pumps","General Appearance","Equipment Related","","","","","ME Fuel pump save oils and area between cylinders has cleaned and painted.","2021-10-17T23:59:35","","Completed","2021-10-17T23:59:35","No","No","No","Internal"]
[null,null,null,22393,null,"122_31-10-2021 19:19:14","2021-10-16T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Oxy/ acetylene gauge glass cover is faded and not clear.to clean","E/R - Pipes/ valves & fittings,Miscellaneous","General Appearance","Equipment Related","","","","","Oxy/ acetylene gauge glass cover removed and cleaned. ","2021-10-31T23:59:35","","Completed","2021-10-18T23:59:35","No","No","No","Internal"]
[null,null,null,22394,null,"122_31-10-2021 19:34:38","2021-10-16T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ME FO Circulating pp discharge pressure gauge faulty ,needs to be renewed","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","","","","","ME FO Circulating pp discharge pressure gauge renewed","2021-10-19T23:59:35","","Completed","2021-10-17T23:59:35","No","No","No","Internal"]
[null,null,null,22395,null,"122_30-10-2021 15:40:57","2021-10-16T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Provision room lobby area floor is not clean & contains water. Floor to be cleaned and kept dry at all times.","Accommodation,Miscellaneous","General Appearance","Equipment Related","","","","","Provision room lobby area floor cleaned and dried. ","2021-11-15T23:59:35","","Completed","2021-10-19T23:59:35","No","No","No","Internal"]
[null,null,null,22396,null,"122_30-10-2021 15:49:00","2021-10-16T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Loose wirings on the bridge to be arranged.","Miscellaneous","General Appearance","Equipment Related,Inappropriate Procedure","","","","","Extra length wiring on bridge to be shortened and loose wiring to be arranged / coiled & secured.","2021-10-23T23:59:35","","Completed","2021-10-23T23:59:35","No","No","No","Internal"]
[null,null,null,22397,null,"122_30-10-2021 16:07:11","2021-10-16T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Mooring winch BRC test dates not stencilled on few mooring winches.","Deck - Mooring Machinery","General Appearance","Inappropriate Procedure","","","","","Stencil the BRC test date on mooring winch.","2021-11-16T23:59:35","","Completed","2021-10-18T23:59:35","No","No","No","Internal"]
[null,null,null,22398,null,"122_30-10-2021 16:37:47","2021-10-16T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Few of the garbage drums kept in garbage storage area needs replacement.","Accommodation","General Appearance","External Factors","","","","","Replaced drums with newly color coded drums.","2021-10-31T23:59:35","","Completed","2021-10-26T23:59:35","No","No","No","Internal"]
[null,null,null,22399,null,"122_31-10-2021 17:01:47","2021-10-16T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ER 15 ppm unit ares found dirty ,needs to be cleaned","Miscellaneous","General Appearance","Equipment Related","","","","","Around 15ppm unit dust removed and soap wash carried out.","2021-10-18T23:59:35","","Completed","2021-10-17T23:59:35","No","No","No","Internal"]
[null,null,null,22400,null,"122_31-10-2021 19:10:58","2021-10-16T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ER logbook few entry like ME fuel rack missing,same to update daily when applicable.Boiler ,cooling water test","Miscellaneous","Cert. & Docu.","Inappropriate Procedure","","","","","Log book entries updated on daily basis. Boiler water tests results included in log book entry","2021-10-17T23:59:35","","Completed","2021-10-17T23:59:35","No","No","No","Internal"]
[null,null,null,22390,null,"122_30-10-2021 17:14:04","2021-10-25T23:59:35","Observation","Ship Staff","Ship Staff Insp.","No. 1 cargo hold hatch cover turnbuckle bolt attached to the chain arm in the aft found rusty and thinned down.","Deck - Machinery","ISM Related","Equipment Related","","","","","The turnbuckle bolt renewed with new one.","2021-12-25T23:59:35","","Completed","2021-11-11T23:59:35","No","No","No","Internal","pls raise RO for new spare"]
[null,null,null,23786,null,"122_17-11-2021 04:07:47","2021-10-27T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Accomodation AC condenser SW inlet pipe section in ER found with pin hole leak.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Pipe section has been removed and fabricated with new pipe section.","2021-11-10T23:59:35","","Completed","2021-10-29T23:59:35","No","No","No","Internal"]
[null,null,null,23787,null,"122_17-11-2021 04:14:23","2021-10-27T23:59:35","Defect","Ship Staff","Ship Staff Insp.","APT sea water in/out pipe section found with pin hole leak.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Pipe section has been removed and fabricated with new pipe section.","2021-11-10T23:59:35","","Completed","2021-11-08T23:59:35","No","No","No","Internal"]
[null,null,null,23788,null,"122_16-11-2021 06:29:51","2021-10-30T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Battery room floor rubber mat found torn and old.","Elect. Mach. & Equip.,Miscellaneous","General Appearance","External Factors","","","","","Renewed the floor rubber mat.","2021-11-03T23:59:35","","Completed","2021-11-02T23:59:35","No","No","No","Internal"]
[null,null,null,23789,null,"122_16-11-2021 07:09:03","2021-10-30T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Mooring drum retention bolt in fwd winches found more than 3 mm","Deck - Mooring Machinery","Mooring","Equipment Related","","","","","Adjusted the retention bolt gap to 2-3 mm.","2021-11-03T23:59:35","","Completed","2021-11-02T23:59:35","No","No","No","Internal"]
[null,null,null,23790,null,"122_16-11-2021 07:30:34","2021-10-30T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Water was found in forecastle store bilges.","Miscellaneous","General Appearance","Inappropriate Procedure","","","","","Bilges were cleaned and dried.","2021-11-03T23:59:35","","Completed","2021-11-01T23:59:35","No","No","No","Internal"]
[null,null,null,23792,null,"122_16-11-2021 07:20:35","2021-10-30T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Tally room floor need painting and clean up.","Accommodation","General Appearance","Inappropriate Procedure","","","","","Tally room cleaned and floor painted. ","2021-11-03T23:59:35","","Completed","2021-11-02T23:59:35","No","No","No","Internal"]
[null,null,null,23791,null,"122_01-01-2022 17:31:38","2021-11-09T23:59:35","Critical Equipment,Defect","Ship Staff","Ship Staff Insp.","Life boat davit hydraulic operational valve block found with oil leak from the end cover during operation.","Miscellaneous","Safety / LSA / FFA","Equipment Related","","","","","Complete Valve block changed with new spare received at Istanbul.","2021-12-26T23:59:35","","Completed","2021-12-25T23:59:35","No","No","No","Internal"]
[null,null,null,23793,null,"122_15-12-2021 00:12:42","2021-11-15T23:59:35","Critical Equipment,Defect","Ship Staff","Ship Staff Insp.","Emergency Generator found  not starting on No.1 set battery, Battery found drained and showing replacement indication.","Elect. Mach. & Equip.","Emgcy. Systems","Equipment Related","","","","","No.1 set battery replaced with new set of battery received at Norfolk.","2021-12-10T23:59:35","","Completed","2021-12-01T23:59:35","No","No","No","Internal"]
[null,null,null,23783,null,"122_01-01-2022 17:13:18","2021-12-12T23:59:35","Defect","Ship Staff","Ship Staff Insp.","ME LO cooler SW inlet and outlet pipe elbows found with pin hole leaks.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Pipe section removed from place and replaced by fabricating new pipe section in Engine Room workshop. Leak fault rectified.","2022-03-26T23:59:35","","Completed","2022-02-24T23:59:35","No","No","No","Internal"]
[null,null,null,21128,null,"122_30/8/2021 10:57:16 pm","2021-12-31T23:59:35","Defect","Ship Staff","Ship Staff Insp.","No.3 Cargo Hold australian ladder rails detached from two locations","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","","","","","Damaged railings cropped & renewed .","2022-06-23T23:59:35","","Completed","2022-05-06T23:59:35","No","No","No","Internal",""]
[null,null,null,21129,null,"122_30/8/2021 11:30:04 pm","2022-01-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Most of the cargo holds have got grab damages, need more close up inspection.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","","","","","Need thickness measurement and severe damage of plate need renewal. DD Specs will be raised in REFMAN","2023-04-25T23:59:35","","Completed","2022-03-26T23:59:35","No","No","No","Internal"]
[null,null,null,21145,null,"122_31/8/2021 6:35:34 pm","2022-01-02T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Hatch cover cleats resting areas found with grooving and washers deformed.","Deck - Machinery","ISM Related","Equipment Related","","","","","Required to remove the plate. DD Specs will be raised.","2023-04-25T23:59:35","","Completed","2022-03-26T23:59:35","No","No","No","Internal"]
[null,null,null,21149,null,"122_17-09-2021 07:50:13","2022-01-02T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Vertical ladder in many cargo holds found slightly deformed due to grab damage.","Cargo Mach.","Structural Condn. / WT integrity ","Equipment Related","","","","","This job to be undertaken during ballast passage. Vessel will plan it in priority order i.e start with hold with ladder in worst condition. Hot work repairs will be carried out.","2022-05-26T23:59:35","","Completed","2022-05-06T23:59:35","No","No","No","Internal","please advise repair plan."]
[null,null,null,21144,null,"122_31/8/2021 6:28:53 pm","2022-01-05T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Wheel lifter hydraulic hoses crimping areas found rusted. Need to check for spare hoses onboard and raise RO\n\naccordingly.","Deck - Machinery","ISM Related","Equipment Related","","","","","Few hydraulic hose found in forcastle store. Received RO for new hose NAQU210030. Damaged hoses renewed.","2022-03-25T23:59:35","NAQU210030","Completed","2022-02-24T23:59:35","No","No","No","Internal"]
[null,null,null,21127,null,"122_30/8/2021 10:42:45 pm","2022-01-08T23:59:35","Defect","Ship Staff","Ship Staff Insp.","No.1 Cargo Hold Australian Ladder Railing Cracked.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","","","","","Railing to be crop & renewed during the ballast passage. Planned for next ballast passage.","2022-05-15T23:59:35","","Completed","2022-05-05T23:59:35","No","No","No","Internal","please update repair plan and progress."]
[null,null,null,21158,null,"122_16-09-2021 07:10:34","2022-01-10T23:59:35","Defect","Ship Staff","Suptd. Insp.","ME AFT air cooler ,Forward end cover sea water leaking.","E/R - Main Engine,E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","ME Aft Air Cooler end cover gasket renewed, Valve replaced with new spare. Leak fault rectified.","2022-03-26T23:59:35","","Completed","2022-02-25T23:59:35","No","No","No","Internal"]
[null,null,null,23785,null,"122_01-02-2022 01:37:59","2022-01-19T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","FW line on main deck found damaged due to ice formation in FW line.","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","Human Error,Inappropriate Procedure","","","","","Damaged sections renewed and all leaks repaired","2022-04-15T23:59:35","","Completed","2022-03-28T23:59:35","No","No","No","Internal"]
[null,null,null,23909,null,"122_16-02-2022 22:59:20","2022-01-27T23:59:35","Observation","Ship Staff","Ship Staff Insp.","FW line on D-deck outside accomodation found damaged and water leaking.","Deck - Pipe / Fittings","MLC Related","External Factors","","","","","The damaged section of pipe to crop out and renew the pipe line section.","2022-04-26T23:59:35","","Completed","2022-02-14T23:59:35","No","No","No","Internal"]
[null,null,null,23913,null,"122_16-02-2022 22:55:07","2022-01-27T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Fire line on deck found leaking at corssdeck of #6 & #7","Deck - Pipe / Fittings","Safety / LSA / FFA","External Factors","","","","","The damaged section of fire cropped out and renewed it and fire line pressure tested and found satisfactory.","2022-04-26T23:59:35","","Completed","2022-02-11T23:59:35","No","No","No","Internal"]
[null,null,null,24584,null,"122_31-03-2022 08:53:15","2022-01-31T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Main Engine forward and aft Air Cooler air leakage.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Main Engine Air Cooler Forward and Aft air side O rings replaced. Air leak fault rectified.","2022-04-29T23:59:35","","Completed","2022-03-03T23:59:35","No","No","No","Internal"]
[null,null,null,23910,null,"122_16-02-2022 12:23:12","2022-01-31T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Main Cooling Sea Water Overboard pipe section found to be leaking from welding Seam.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Main CSW overboard pipe section replaced with new pipe section fabricated in Engine Room workshop. Leak fault rectified. ","2022-04-29T23:59:35","","Completed","2022-03-17T23:59:35","No","No","No","Internal"]
[null,null,null,23914,null,"122_16-02-2022 12:17:19","2022-02-08T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Aux Engine no. 2 Starting Air pressure regulating valve not regulating pressure, Aux Engine starting air pressure rising above normal value of 7 to 10 Bar.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Aux. Engine no. 2 Pressure regulating valve opened up for inspection and repair. Valve seat spindle found to be damaged and diaphragm not sealing completely. Valve Seat and Diaphragm replaced with new spare available. Regulating Valve tried out after overhaul and cleaning, air pressure fault rectified, perfromance satisfactory.","2022-05-07T23:59:35","","Completed","2022-02-09T23:59:35","No","No","No","Internal"]
[null,null,null,23911,null,"122_16-02-2022 23:04:51","2022-02-09T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Hatch cover no. 6 drive wire turnbuckle conneting to the chain arm was found broken / parted.","Cargo Mach.","Cargo / Ballast Systems","External Factors","","","","","Renewed the turnbuckle and connected back the drive wire to the chain arm.","2022-05-09T23:59:35","","Completed","2022-02-11T23:59:35","No","No","No","Internal"]
[null,null,null,23915,null,"122_16-02-2022 12:00:31","2022-02-09T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Boiler Water low level alarm coming repeatedly during Engine Room UMS","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","Boiler water level low because of Automatic pneumatic level controller valve not opening completely. Valve Controller opened up for inspection and repair, found O Ring damaged on Pneumatic Valve controller shaft, all O rings replaced with new spare. Defect rectified, Boiler level controller performance satisfactory.","2022-05-07T23:59:35","","Completed","2022-02-09T23:59:35","No","No","No","Internal"]
[null,null,null,23912,null,"122_16-02-2022 23:09:33","2022-02-10T23:59:35","Defect","Ship Staff","Ship Staff Insp.","The wheel house window wash pipeline nozzles are choked.","Deck - Pipe / Fittings","Navigation","External Factors","","","","","Isolate the wheel house window wash pipeline and open up the noozles to clear the line. All lines have been cleared and window wash operation is satisfactory.","2022-05-10T23:59:35","","Completed","2022-03-19T23:59:35","No","No","No","Internal"]
[null,null,null,24144,null,"122_02-03-2022 12:18:01","2022-02-12T23:59:35","Defect","Ship Staff","Ship Staff Insp.","FO Service tank heating steam inlet valve not holding and spindle in broken condition","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","FO service tank heating steam inlet valve replaced with new spare available, fault rectified.","2022-05-13T23:59:35","","Completed","2022-02-23T23:59:35","No","No","No","Internal"]
[null,null,null,24145,null,"122_02-03-2022 12:21:37","2022-02-12T23:59:35","Defect","Ship Staff","Ship Staff Insp.","FO Bunker Tank 2P heating steam inlet valve not holding","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","FO Bunker Tank 2P heating steam inlet valve removed from place and valve seat lapping carried out, fault rectified.","2022-05-13T23:59:35","","Completed","2022-02-23T23:59:35","No","No","No","Internal"]
[null,null,null,24582,null,"122_31-03-2022 08:48:15","2022-02-20T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Main Engine LO Cooler SW outlet pipe section leaking from seam.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Main Engine LO Cooler SW outlet pipe section replaced with new pipe section fabricated in Engine Room workshop.","2022-05-19T23:59:35","","Completed","2022-02-24T23:59:35","No","No","No","Internal"]
[null,null,null,24142,null,"122_02-03-2022 12:02:43","2022-02-23T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Aux Engine JW cooler no. 1 SW inlet pipe leak from pin hole","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Aux Engine JW Cooler 1 leaking SW inlet pipe repaired by hot work welding in Engine Room workshop.","2022-05-27T23:59:35","","Completed","2022-04-02T23:59:35","No","No","No","Internal"]
[null,null,null,24143,null,"122_02-03-2022 12:08:15","2022-02-24T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Main Engine JW Cooler SW outlet pipe leak from pin hole","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Main Engine JW Cooler SW outlet pipe section replaced with new pipe section fabricated in Engine Room Workshop.","2022-04-26T23:59:35","","Completed","2022-03-17T23:59:35","No","No","No","Internal"]
[null,null,null,24583,null,"122_31-03-2022 08:43:04","2022-02-28T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Main CSW pump no. 1 discharge valve not holding.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Discharge valve opened up for inspection and repairs, found valve spindle broken. Valve spindle repaired in Engine Room workshop, fault rectified.","2022-05-31T23:59:35","","Completed","2022-03-17T23:59:35","No","No","No","Internal"]
[null,null,null,24579,null,"122_31-03-2022 07:33:19","2022-03-15T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Fire line on main deck between cross deck of #1 & #2 found hole.","Deck - Pipe / Fittings","Safety / LSA / FFA","Equipment Related","","","","","Pipe section renewed","2022-06-15T23:59:35","","Completed","2022-04-05T23:59:35","No","No","No","Internal"]
[null,null,null,24580,null,"122_31-03-2022 07:02:06","2022-03-18T23:59:35","Defect","Ship Staff","Ship Staff Insp.","No. 1 TST (P) tank plate where filling pipe from bottom tank joins the TST thinned down and wasted and water is seeping into the cargo hold no. 1.","Hull & Tanks","Cargo / Ballast Systems","External Factors","","","","","Permanent repairs carried by hot work after seeking hot work approval.the crack is been built up and thinned down plate renewed.","2022-06-18T23:59:35","","Completed","2022-04-28T23:59:35","No","No","No","Internal"]
[null,null,null,24581,null,"122_31-03-2022 07:20:58","2022-03-18T23:59:35","Defect","Ship Staff","Ship Staff Insp.","No. 5 TST (P) tank plate where filling pipe from bottom tank joins the TST thinned down and wasted and water is seeping into the cargo hold no. 7.","Hull & Tanks","Cargo / Ballast Systems","External Factors","","","","","permenant repairs carried out by hot work . crack built up and plate welded to seal the thinned down plating.protective caoting applied. after drying out of paint, tank filled up and checked for leakage, satifsfactory.","2022-06-18T23:59:35","","Completed","2022-05-03T23:59:35","No","No","No","Internal"]
[null,null,null,24965,null,"122_18-04-2022 14:35:09","2022-04-09T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Main LO Cooler SW inlet pipe leaking from flange welding seam","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Main LO Cooler SW inlet pipe section removed and new pipe fabricated in ER workshop. protective caoting applied from inside. after drying, pipe fitted back in place.","2022-07-09T23:59:35","","Completed","2022-04-19T23:59:35","No","No","No","Internal"]
[null,null,null,24966,null,"122_18-04-2022 21:00:50","2022-04-12T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Hatch cover no. 6 fwd (s)- Hydraulic oil leaking from lifting jack. ","Deck - Machinery","ISM Related","Equipment Related","","","","","leaky jack replaced with overhauled jack, system tested for operation. found satisfactory without leak","2022-07-12T23:59:35","","Completed","2022-05-04T23:59:35","No","No","No","Internal"]
[null,null,null,25687,null,"122_14/6/2022 8:40:38 pm","2022-04-19T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Reefer Rom lobby defrosting need to be checked. Found lot of icing.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","The lobby evaporator coil has no Defrost heater. Manual defrosting carried using hot water on weekly basis. Ship staff will carry out defrosting every alternate day.\n\n","2022-05-19T23:59:35","","Completed","2022-04-27T23:59:35","No","No","No","Internal"]
[null,null,null,25688,null,"122_14/6/2022 8:50:36 pm","2022-04-19T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","oxy and acetylene flame arrestor and flash back arrestor in bad shape. Need renewal . \n\nhosses for both near torch  is showing cracks. \n\n","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Oxy and Acetylene flash back arrestors replaced.crack hose replaced. Replacement carried after receiving Unitor stores.","2022-05-19T23:59:35","NAQU220067","Completed","2022-06-06T23:59:35","No","No","No","Internal"]
[null,null,null,25689,null,"122_14/6/2022 8:54:29 pm","2022-04-19T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Lifting gear maintenance or checks are not displayed near the chain blocks and slings","Documentation","ISM Related","Human Error,Inappropriate Procedure","","","","","Lifting gear checklist sheet displayed near lifting gear stored area","2022-05-09T23:59:35","","Completed","2022-05-05T23:59:35","No","No","No","Internal"]
[null,null,null,25690,null,"122_14/6/2022 9:40:08 pm","2022-04-19T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Welding cable has few soft patches(tapes) discard and order if new is required. ","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","Welding cable was damaged at clamp end, same cropped and repaired.","2022-05-19T23:59:35","","Completed","2022-05-15T23:59:35","No","No","No","Internal"]
[null,null,null,25691,null,"122_14/6/2022 9:49:00 pm","2022-04-19T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Acy room reducer pressure gauge is damaged. Last changed records not found. ","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Acetylene room pressure reducing unit replaced afetr recieving Unitor stores.","2022-05-19T23:59:35","NAQU220067","Completed","2022-06-06T23:59:35","No","No","No","Internal"]
[null,null,null,25692,null,"122_14/6/2022 9:51:44 pm","2022-04-19T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Oxy room reducer and flash back arrestor last installed renewed records are not available. Need replacement. ","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Oxygen room pressure reducing valve and flash back arrestors replaced.","2022-06-19T23:59:35","NAQU220067","Completed","2022-06-06T23:59:35","No","No","No","Internal"]
[null,null,null,25693,null,"122_14/6/2022 9:54:25 pm","2022-04-19T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","No 6 Hyd jack leaking – 1 set ","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","CH-6 leaky jack removed and leak rectified by replacing wasted out vent plug.","2022-05-19T23:59:35","","Completed","2022-05-04T23:59:35","No","No","No","Internal"]
[null,null,null,25694,null,"122_14/6/2022 9:56:37 pm","2022-04-19T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Fore peak store Ballast valve not operational. ","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","","","","","valve actuator removed and overhauled, now working satisfactory in manual and remote operation modes.","2022-05-19T23:59:35","","Completed","2022-04-19T23:59:35","No","No","No","Internal"]
[null,null,null,25695,null,"122_14/6/2022 9:59:28 pm","2022-04-19T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Port side gangway platform is damaged/bent. SWL not mentioned. ","Deck - Machinery","Structural Condn. / WT integrity ","Equipment Related","","","","","the wasted out chequered plate cropped and plate support removed. New supports fabricated. new chequered plate fitted in place","2022-06-19T23:59:35","","Completed","2022-04-22T23:59:35","No","No","No","Internal"]
[null,null,null,25696,null,"122_14/6/2022 8:46:20 pm","2022-04-19T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Flame Screen in workshop is damaged","Miscellaneous","Eng. / Strg. Comp.","Inappropriate Procedure","","","","","Flame screen renewed after recieving Unitor store.","2022-05-19T23:59:35","NAQU220067","Completed","2022-07-06T23:59:35","No","No","No","Internal"]
[null,null,null,25697,null,"122_14/6/2022 10:12:38 pm","2022-04-19T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Test report of LSMGO not posted in ECR","Documentation","Cert. & Docu.","Inappropriate Procedure","","","","","The LSMGO fuel oil analysis report is posted in ECR. Ship staff briefed to follow the procedure of posting latest fuel oil analysis reports when received for easy reference.","2022-04-24T23:59:35","","Completed","2022-04-21T23:59:35","No","No","No","Internal"]
[null,null,null,25698,null,"122_14/6/2022 10:14:39 pm","2022-04-19T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ECR UMS CL does not made vessel specific","Documentation","Cert. & Docu.","Inappropriate Procedure","","","","","Generic UMS checklist in PAL amended and made vessel specific.","2022-05-09T23:59:35","","Completed","2022-04-21T23:59:35","No","No","No","Internal"]
[null,null,null,25699,null,"122_14/6/2022 10:18:09 pm","2022-04-19T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ECR Black out recovery procedure not made. Manual copy only posted. ","Documentation","ISM Related","Inappropriate Procedure","","","","","ship specific Black out recovery procedure made and discussed with engine staff. Same posted in ECR","2022-05-19T23:59:35","","Completed","2022-04-21T23:59:35","No","No","No","Internal"]
[null,null,null,25700,null,"122_14/6/2022 10:19:56 pm","2022-04-19T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Electric shock first aid procedure not posted. ","Documentation","ISM Related","Inappropriate Procedure","","","","","The poster provided by GOODWOOD is posted in ECR, staff briefed about the procedure","2022-05-19T23:59:35","","Completed","2022-04-28T23:59:35","No","No","No","Internal"]
[null,null,null,25701,null,"122_14/6/2022 10:24:34 pm","2022-04-19T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Seals present on OWS to OVBD line flanges are painted. Seal numbers should be visible. Either remove paint or replace seals. ","Miscellaneous","Eng. / Strg. Comp.","Inappropriate Procedure","","","","","OWS overboard line seal checked and paint on seal cleaned, the seal numbers are visible.","2022-05-19T23:59:35","","Completed","2022-04-25T23:59:35","No","No","No","Internal"]
[null,null,null,25702,null,"122_14/6/2022 10:29:37 pm","2022-04-19T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","STP By pass valve was found to be open and not sealed in PORT. ","Miscellaneous","Eng. / Strg. Comp.","Inappropriate Procedure","","","","","Crew briefed about not to bypass the STP onboard. Poster put at the valve location. ","2022-05-09T23:59:35","","Completed","2022-04-26T23:59:35","No","No","No","Internal"]
[null,null,null,25703,null,"122_14/6/2022 10:31:26 pm","2022-04-19T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","PAL PMS Jobs are pending since Jan 2022. Same needs to be updated","Documentation","Cert. & Docu.","Inappropriate Procedure","","","","","All pending jobs completed and updated in PAL.","2022-05-19T23:59:35","","Completed","2022-05-19T23:59:35","No","No","No","Internal"]
[null,null,null,25704,null,"122_14/6/2022 10:10:36 pm","2022-04-19T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","AHU filters to clean","Miscellaneous","Eng. / Strg. Comp.","Inappropriate Procedure","","","","","AHU return air filters cleaning carried. Weekly cleaning routine is proposed to ship staff.","2022-05-04T23:59:35","","Completed","2022-04-26T23:59:35","No","No","No","Internal"]
[null,null,null,25705,null,"122_14/6/2022 10:21:43 pm","2022-04-19T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Few Places Electrical mats in bottom platform missing","Miscellaneous","Eng. / Strg. Comp.","Inappropriate Procedure","","","","","Electrical insulation mats placed below starter panels.","2022-05-19T23:59:35","","Completed","2022-05-01T23:59:35","No","No","No","Internal"]
[null,null,null,25706,null,"122_15/6/2022 1:41:26 am","2022-04-19T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Few rollers on deck, greasing required.","Deck - Mooring Machinery","Mooring","Equipment Related","","","","","Roller greasing carried out ,old grease removed and cleaned new grease filled.","2022-05-04T23:59:35","","Completed","2022-05-04T23:59:35","No","No","No","Internal"]
[null,null,null,25707,null,"122_15/6/2022 1:58:35 am","2022-04-19T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","fed wheels need greasing and cleaning","Deck - Mooring Machinery","Mooring","Equipment Related","","","","","Fed Wheels cleaned old greased removed and new greasing carried out","2022-05-19T23:59:35","","Completed","2022-05-16T23:59:35","No","No","No","Internal"]
[null,null,null,25708,null,"122_15/6/2022 2:00:52 am","2022-04-19T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","All reefer room need cleaning.","Miscellaneous","General Appearance","Inappropriate Procedure","","","","","Refer room cleaning carried out and stores arranged","2022-05-03T23:59:35","","Completed","2022-04-29T23:59:35","No","No","No","Internal"]
[null,null,null,25709,null,"122_15/6/2022 2:03:07 am","2022-04-19T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","SWL on pilot ladder not mentioned. ","Deck - Machinery","General Appearance","Inappropriate Procedure","","","","","Pilot Assist ladder port and stbd side Platform upper and lower , stenciled","2022-05-19T23:59:35","","Completed","2022-05-16T23:59:35","No","No","No","Internal"]
[null,null,null,25710,null,"122_15/6/2022 2:05:37 am","2022-04-19T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Mooring winch operating control blocks to be covered with canvas","Deck - Mooring Machinery","Mooring","External Factors","","","","","Canvas cover prepared for all mooring winch operating control box and covered it.","2022-05-10T23:59:35","","Completed","2022-05-09T23:59:35","No","No","No","Internal"]
[null,null,null,25714,null,"122_14/6/2022 10:35:20 pm","2022-04-19T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Calculation of ROB required for EDE to run for min 18 hours should be taken form manual and posted. Marking a point in gauge glass without evidence is not acceptable by 3rd party inspections many times. Same goes for steering gear. ","Documentation","Eng. / Strg. Comp.","Inappropriate Procedure","","","","","makers manual referred and max consumption at 100% load obtained. Minimum fuel required for 18 hrs use calculated and found to be 388.6 liters for emergency generator. The load test printout posted with calculation on emergency generator fuel oil tank. minimum fuel level marked correctly.\n\n\n\n","2022-05-19T23:59:35","","Completed","2022-04-25T23:59:35","No","No","No","Internal"]
[null,null,null,25711,null,"122_30/4/2022 12:21:31 pm","2022-04-20T23:59:35","Defect","Class Surveyor","Others (Eg. Insurance etc.)","class NK surveyor had pointed out the port side accommodation ladder upper platform's chequered plate is watesd out at various location.","Deck - Machinery","Structural Condn. / WT integrity ","Equipment Related","","","","","the material required to carry out repair was connected at Hazira and repairs are carried out after departure. the support structure and chequred plate are renewed and report sent to class.","2022-04-22T23:59:35","","Completed","2022-04-22T23:59:35","No","No","No","External"]
[null,null,null,25712,null,"122_14/6/2022 8:37:41 pm","2022-04-20T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","pipes need securing in ECR deck","Miscellaneous","Eng. / Strg. Comp.","Inappropriate Procedure","","","","","Spare Pipes in machinery space secured properly. Packings put to avoid movement of spare pipes during heavy weather.","2022-05-19T23:59:35","","Completed","2022-04-25T23:59:35","No","No","No","Internal"]
[null,null,null,25713,null,"122_15/6/2022 2:10:59 am","2022-04-30T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","CRA for Liberia Seaman Book of 3/E and Original Liberian Flag state endorsement of 4/E not onboard.","Documentation","Cert. & Docu.","External Factors","","","","","CRA for both officers has been rcvd.","2022-05-31T23:59:35","","Completed","2022-05-07T23:59:35","No","No","No","Internal"]
[null,null,null,25715,null,"122_15/6/2022 2:13:35 am","2022-04-30T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Stbd Bunker hose crane and Port Provision Crane hooks secured with Wire instead of rope. ","Deck - Machinery","Safety / LSA / FFA","Human Error","","","","","Stbd and Port Bunker hose crane and Port Provision Crane hooks replaced wire rope securing with Tiger rope","2022-05-31T23:59:35","","Completed","2022-05-21T23:59:35","No","No","No","Internal"]
[null,null,null,25716,null,"122_15/6/2022 2:15:50 am","2022-04-30T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","All loose drums and materials kept on exterior accommodation especially on D Deck to wire lash. ","Accommodation","Safety / LSA / FFA","Human Error","","","","","All Drums on D Deckwirelashed with bottle screw ","2022-05-31T23:59:35","","Completed","2022-05-21T23:59:35","No","No","No","Internal"]
[null,null,null,25717,null,"122_15/6/2022 2:20:32 am","2022-04-30T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Few Antennas on Monkey Island is not identified and stenciled. ","Miscellaneous","General Appearance","Inappropriate Procedure","","","","","Antennas on Monkey Island  identified and stenciled. ","2022-06-07T23:59:35","","Completed","2022-06-06T23:59:35","No","No","No","Internal"]
[null,null,null,25718,null,"122_15/6/2022 2:23:27 am","2022-04-30T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Engine room blowers near primary muster station require cosmetic upgradation.","Elect. Mach. & Equip.","General Appearance","External Factors","","","","","Engine room blowers near primary muster station Port and Stbd rust weepings removed by rust remover ","2022-06-15T23:59:35","","Completed","2022-05-29T23:59:35","No","No","No","Internal"]
[null,null,null,25719,null,"122_15/6/2022 2:25:29 am","2022-04-30T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Securing chains for MF/HF Antenna on Monkey Island in poor condition.","Miscellaneous","General Appearance","Equipment Related","","","","","Securing chains for MF/HF Antenna on Monkey Island derusted and painted","2022-05-31T23:59:35","","Completed","2022-05-29T23:59:35","No","No","No","Internal"]
[null,null,null,25720,null,"122_15/6/2022 2:27:27 am","2022-04-30T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Empty Oxygen and Acetylene bottles kept near Port side gangway to secure with wire lashings.","Miscellaneous","Safety / LSA / FFA","External Factors","","","","","Empty Oxygen and Acetylene bottles kept near Port side gangway  secured with wire lashings","2022-05-31T23:59:35","","Completed","2022-05-25T23:59:35","No","No","No","Internal"]
[null,null,null,25721,null,"122_15/6/2022 2:29:44 am","2022-04-30T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Photographic starting procedures to be made for the following equipment’s: Fixed Foam Firefighting system, Hyper mist system, Quick closing valves, BA Compressor.","Critical Equip.","Eng. / Strg. Comp.","Inappropriate Procedure","","","","","Photographic starting procedures  made for the following equipment’s: Fixed Foam Firefighting system, Hyper mist system, Quick closing valves, BA Compressor.","2022-06-09T23:59:35","","Completed","2022-06-06T23:59:35","No","No","No","Internal"]
[null,null,null,25722,null,"122_15/6/2022 2:31:27 am","2022-04-30T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Proper securing and storage arrangement to be made for BA Compressor.","Critical Equip.","Emgcy. Systems","Equipment Related","","","","","Proper securing and storage arrangement for BA Compressor made in Emergency Generator room","2022-05-31T23:59:35","","Completed","2022-05-29T23:59:35","No","No","No","Internal"]
[null,null,null,25723,null,"122_15/6/2022 2:33:34 am","2022-04-30T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","MSDS for the Foam solution to be posted at all portable foam applicator sets.","Documentation","Cert. & Docu.","Inappropriate Procedure","","","","","MSDS Foam solution posted on 20 ltrs (2 nos) Foam Applicator in SOPEP locker & Eng Rm first platform","2022-05-31T23:59:35","","Completed","2022-05-21T23:59:35","No","No","No","Internal"]
[null,null,null,25724,null,"122_15/6/2022 2:44:19 am","2022-04-30T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","FFA training manual does not contain information about BA Compressor.","Critical Equip.","Emgcy. Systems","Inappropriate Procedure","","","","","Ship Specific BA Compressor operating instructions attached in FFA training manuals Crew & officer Smoke and Mess Rooms","2022-05-31T23:59:35","","Completed","2022-05-21T23:59:35","No","No","No","Internal"]
[null,null,null,25725,null,"122_15/6/2022 2:46:15 am","2022-04-30T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Metal frame for Hotplate in Galley is corroded and choked.","Miscellaneous","General Appearance","Equipment Related","","","","","All Metal frames for hotplates in galley Degreased cleaned and derusted","2022-06-15T23:59:35","","Completed","2022-05-25T23:59:35","No","No","No","Internal"]
[null,null,null,25726,null,"122_15/6/2022 2:48:24 am","2022-04-30T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Forepeak store Eductor line diagram to be posted at location.","Documentation","Emgcy. Systems","Inappropriate Procedure","","","","","Fore Peak store Eductor Diagram posted on Port and stbd Bulkhead near Bilge well","2022-05-31T23:59:35","","Completed","2022-05-25T23:59:35","No","No","No","Internal"]
[null,null,null,25727,null,"122_15/6/2022 2:50:20 am","2022-04-30T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","No rubber matting below welding equipment in forecastle.","Deck - Machinery","Safety / LSA / FFA","Inappropriate Procedure","","","","","Rubber matting placed below welding equipment ","2022-05-31T23:59:35","","Completed","2022-05-25T23:59:35","No","No","No","Internal"]
[null,null,null,25728,null,"122_15/6/2022 11:51:52 pm","2022-04-30T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","3 nos taps in Galley not working and operated by the main stop valve.","Miscellaneous","General Appearance","Equipment Related","","","","","Leaky taps repaired and now operable.","2022-05-31T23:59:35","","Completed","2022-05-27T23:59:35","No","No","No","Internal"]
[null,null,null,25729,null,"122_15/6/2022 11:54:36 pm","2022-04-30T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Guards missing on all pumps in Engine room.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","","","","","Guards made in ER workshop and placed on all large pumps","2022-05-31T23:59:35","","Completed","2022-05-26T23:59:35","No","No","No","Internal"]
[null,null,null,25730,null,"122_15/6/2022 2:37:54 am","2022-04-30T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Port Bunker davit Slewing mechanism to make free and grease.","Deck - Machinery","Cargo / Ballast Systems","Equipment Related","","","","","Port Bunker davit Slewing mechanism freed and greased.","2022-05-31T23:59:35","","Completed","2022-05-22T23:59:35","No","No","No","Internal"]
[null,null,null,25731,null,"122_15/6/2022 11:56:42 pm","2022-04-30T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Loose items behind G/E FO Circulating pump to secure.","Miscellaneous","Eng. / Strg. Comp.","Inappropriate Procedure","","","","","All loose items secured properly.","2022-05-31T23:59:35","","Completed","2022-05-19T23:59:35","No","No","No","Internal"]
[null,null,null,25732,null,"122_16/6/2022 12:01:48 am","2022-04-30T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Filling pipe from DB Tank to TST Tank have leak in cargo hold as follows: 5S TST to Cargo hold no 7 and 1P TST to Cargo hold no 1.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","","","","","Wasted out plate bult up using hot work, additional plat fabricated to rectify the leak, protective coating applied on new plate. after drying out, tank filled and leak checked, satisfactory.","2022-05-31T23:59:35","","Completed","2022-05-03T23:59:35","No","No","No","Internal"]
[null,null,null,25733,null,"122_16/6/2022 12:03:48 am","2022-04-30T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","MSDS for Oil Spill Dispersants – YCC Blue Clean to be posted in SOPEP Locker.","Documentation","Safety / LSA / FFA","Inappropriate Procedure","","","","","YCC Blue clean removed from Sopep locker/ vsl having FALCHEM OSD with MSDS posted inside Sopep locker","2022-05-31T23:59:35","","Completed","2022-05-19T23:59:35","No","No","No","Internal"]
[null,null,null,25734,null,"122_16/6/2022 12:09:43 am","2022-04-30T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Paint drums kept in the upper rack of Paint store is not secured.","Miscellaneous","Safety / LSA / FFA","Human Error,Inappropriate Procedure","","","","","Paint Drums Arranged and Secured in Upper Rack ","2022-05-31T23:59:35","","Completed","2022-05-31T23:59:35","No","No","No","Internal"]
[null,null,null,25735,null,"122_16/6/2022 12:11:42 am","2022-04-30T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Loose plates and pipes kept near the Port side Gangway to be secured.","Miscellaneous","Safety / LSA / FFA","Human Error,Inappropriate Procedure","","","","","All plates and pipes received in Hazira ,India shifted to f’castle store","2022-04-30T23:59:35","","Completed","2022-05-07T23:59:35","No","No","No","Internal"]
[null,null,null,25736,null,"122_16/6/2022 12:14:23 am","2022-04-30T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","S-Band Radar Performance Monitor box is not operational.","Navigation - Others","Navigation","Equipment Related","","","","","PM box renewed. PM operational.","2022-05-31T23:59:35","","Completed","2022-05-15T23:59:35","No","No","No","Internal"]
[null,null,null,25737,null,"122_16/6/2022 12:16:36 am","2022-04-30T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","MF/HF Unit of GMDSS Console is displaying ATU and PA Load error.","Navigation - GMDSS & Communication","Navigation","Equipment Related","","","","","Burnt PCB renewed. MF/HF operational.","2022-05-31T23:59:35","","Completed","2022-05-31T23:59:35","No","No","No","Internal"]
[null,null,null,25738,null,"122_16/6/2022 12:20:14 am","2022-04-30T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Greasing of Hatch cover rollers, wires to carry out.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","Greasing of Hatch Cover Rollers , wires carried out","2022-06-01T23:59:35","","Completed","2022-06-01T23:59:35","No","No","No","Internal"]
[null,null,null,25739,null,"122_16/6/2022 12:05:50 am","2022-04-30T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Heavy items in Forecastle store to Wire lash.","Miscellaneous","Safety / LSA / FFA","Inappropriate Procedure","","","","","Heavy items in Forecastle store to Wire lash.","2022-05-31T23:59:35","","Completed","2022-05-31T23:59:35","No","No","No","Internal"]
[null,null,null,25740,null,"122_16/6/2022 12:07:21 am","2022-04-30T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","MSDS for Bunker samples to be put in Paint store.","Documentation","Cert. & Docu.","Inappropriate Procedure","","","","","MSDS placed for bunker samples in paint room","2022-05-31T23:59:35","","Completed","2022-05-23T23:59:35","No","No","No","Internal"]
[null,null,null,25686,null,"122_16/6/2022 12:39:16 am","2022-06-08T23:59:35","Observation","Ship Staff","Ship Staff Insp.","poop deck stbd side accommodation entrance door closing damper link bent and not functioning properly","Accommodation","Safety / LSA / FFA","Equipment Related","","","","","poop deck stbd side accommodation entrance door closing damper link  straighten and made it functional.","2022-08-26T23:59:35","","Completed","2022-06-26T23:59:35","No","No","No","Internal"]
[null,null,null,25929,null,"122_30/6/2022 3:49:33 pm","2022-06-15T23:59:35","Defect","Ship Staff","Ship Staff Insp.","AE jacket water cooler-1 , sea water inlet pipe having sea water leakage due to wasted out pipe at near weld seam.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","AE jacket water cooler-1 , sea water inlet pipe removed and jig made, new pipe fabricated and epoxy coating applied internally. after drying out, the new pipe fitted in place and system tried out.","2022-08-25T23:59:35","","Completed","2022-06-16T23:59:35","No","No","No","Internal"]
[null,null,null,25930,null,"122_30/6/2022 3:52:59 pm","2022-06-15T23:59:35","Defect","Ship Staff","Ship Staff Insp.","AE jacket water cooler-2 , sea water inlet pipe having sea water leaking due to wasted out pipe stub, was repaired temporarily.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","AE jacket water cooler-2 , sea water inlet pipe removed and jig made, new pipe fabricated and epoxy coating applied internally. pipe fitted after drying of protective coating. system tried out, satisfactory.","2022-08-25T23:59:35","","Completed","2022-06-16T23:59:35","No","No","No","Internal"]
[null,null,null,25931,null,"122_30/6/2022 3:56:32 pm","2022-06-15T23:59:35","Defect","Ship Staff","Ship Staff Insp.","ME jacket water cooler , sea water inlet stub pipe found having pin hole and is leaking.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","ME jacket water cooler-1 , sea water inlet pipe leaky stub piece removed and new pipe fabricated, epoxy coating applied and pipe fitted back in place. system tried out, satisfactory.","2022-08-25T23:59:35","","Completed","2022-06-23T23:59:35","No","No","No","Internal"]
[null,null,null,26126,96011,"122_Fri Jul 15 2022 16:17:55 GMT+0800","2022-07-01T23:59:35","Observation","Ship Staff","Ship Staff Insp.","dump condenser sea water inlet pipe is leaking from weld seam and pipe seems to be wasted out.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","pipe removed and jig fabricated, removed pipe fitted back and steam system normalized.\non 15-Jul-2022, new pipe fabricated and painted with epoxy inside the pipe walls. pipe fitted in place and tried out, satisfactory.","2022-07-25T23:59:35","","Completed","2022-07-11T23:59:35","No","No","No","Internal",""]
[null,null,null,26125,71270,"122_Mon Jul 11 2022 02:21:35 GMT+0800","2022-07-02T23:59:35","Observation","Ship Staff","Ship Staff Insp.","FWG ejector pump discharge piping having leak at pipe bend.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","pipe removed and inspection carried. jig made and new pipe fabricated, epoxy coating applied till reach and fitted after drying.","2022-10-02T23:59:35","","Completed","2022-07-12T23:59:35","No","No","No","Internal","noted. please update after completion of repair."]
[null,null,null,26128,39969,"122_Mon Jul 11 2022 02:19:46 GMT+0800","2022-07-02T23:59:35","Observation","Ship Staff","Ship Staff Insp.","FWG ejector pump suction line is leaking from weld seam","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","FWG ejector pump leaky suction line removed and weld seam built up carried at ER workshop. pipe fitted back and tried out. leak rectified.","2022-09-25T23:59:35","","Completed","2022-07-04T23:59:35","No","No","No","Internal"]
[null,null,null,26127,56657,"122_Mon Jul 11 2022 20:23:52 GMT+0800","2022-07-05T23:59:35","Observation","Ship Staff","Ship Staff Insp.","AE JW cooler no-1 sea water inlet line is wasted out at various locations and is leaking.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","AE JW cooler-1 isolated and leaky pipe removed, jig made and new pipe fabricated in ER workshop. fitted in place with new gaskets and tried out. ","2022-09-06T23:59:35","","Completed","2022-07-06T23:59:35","No","No","No","Internal"]
[null,null,null,26315,35113,"122_Wed Jul 20 2022 15:03:02 GMT+0800","2022-07-14T23:59:35","Observation","Ship Staff","Ship Staff Insp.","fire and GS pump discharge line to aft peak tank filling is having pin hole and is leaking.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","the leaky pipe removed and repaired in ER workshop. epoxy coating applied and after drying out, pipe fitted back in place. tried out and satisfactory with no leak.","2022-08-26T23:59:35","","Completed","2022-07-15T23:59:35","No","No","No","Internal"]
[null,null,null,23784,null,"122_01-01-2022 17:06:58","2022-07-15T23:59:35","Defect","Ship Staff","Ship Staff Insp.","AE FO viscocity controller found not operational due to faulty PCB","E/R - Aux. Engine,Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","Spares received and renewed controller, found operational.","2022-10-14T23:59:35","NAQU220006","Completed","2022-10-05T23:59:35","No","No","No","Internal","Spare was ready , will connect to vessel at convenient port."]
[null,null,null,26314,84249,"122_Sun Jul 31 2022 03:49:13 GMT+0800","2022-07-18T23:59:35","Observation","Ship Staff","Ship Staff Insp.","ME Turbocharger no-2 grit washing line was observed to be clogged. ME  TC dry washing is not possible due to this clogging.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","ME Turbocharger no-2 grit washing line removed and clogged grit lump was removed, line cleared and crew briefed about back flushing of the grit washing line as per maker's guidelines.","2022-07-26T23:59:35","","Completed","2022-07-21T23:59:35","No","No","No","Internal"]
[null,null,null,26481,85868,"122_Sat Aug 13 2022 20:34:22 GMT+0800","2022-07-28T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Routine running of rescue boat outboard engine ,it was observed that the gear is not engaging in ahead direction, remote direction control box is opened for inspection and found that the shifting cable lug (made of plastic) is cracked and the shifting cable is out of lug.","Critical Equip.","Safety / LSA / FFA","Equipment Related","","","","","Rescue boat outboard engine, remote direction control box shifting cable lug made of plastic replaced with fabricated metal cable lug , after complete box back engine tried out in both ahead and astern using remote direction control box . working satisfactory.","2022-08-26T23:59:35","","Completed","2022-07-29T23:59:35","No","No","No","Internal"]
[null,null,null,25684,null,"122_16/6/2022 12:32:20 am","2022-08-08T23:59:35","Observation","Ship Staff","Ship Staff Insp.","service fresh water valve leaking internally.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","leaky service water valve to overhauled.","2022-10-24T23:59:35","","Completed","2022-09-27T23:59:35","No","No","No","Internal","please advise working plan."]
[null,null,null,26660,82068,"122_Wed Aug 24 2022 01:06:58 GMT+0800","2022-08-13T23:59:35","Defect","Ship Staff","Ship Staff Insp.","ME fuel oil flow meter is giving erratic/wrong readings","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","ME FO flow meter opened up and inspected, found that the locking for the magnetic disc securing to the the shaft sleeve (brass) was worn and magnet having relative movement with gear shaft causing wrong /erratic reading, same rectified.  boxed back in place and observed whilst ME in operation, compared with actual consumption by manually taking service tank sounding, confirmed working satisfactory.   ","2022-09-26T23:59:35","","Completed","2022-08-19T23:59:35","No","No","No","Internal"]
[null,null,null,25928,null,"122_30/6/2022 4:00:01 pm","2022-08-15T23:59:35","Observation","Ship Staff","Ship Staff Insp.","main cooling sea water pump no-1 discharge pipe is having sea water leakage at weld seam due to pin hole.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","leaky pipe to be removed and replaced with new fabricated pipe.\nInlet & outlet valves renewed. Tried out, all operational.","2022-10-25T23:59:35","","Completed","2022-10-19T23:59:35","No","No","No","Internal","please order valves and replace it. stop leakage firstly. please advise RO serial number for valves for office tracking."]
[null,null,null,26659,44630,"122_Tue Aug 30 2022 16:30:57 GMT+0800","2022-08-26T23:59:35","Defect","Ship Staff","Ship Staff Insp.","110v Low insulation traced to fwd mast's aft facing lightings. lighting fixtures observed to be wasted out appreciably and water integrity is lost and seepage is suspected.","Elect. Mach. & Equip.","Navigation","Equipment Related","","","","","low insulation issue rectified, lighting fixtures replaced to avoid reoccurrence of low insulation.","2022-09-26T23:59:35","","Completed","2022-08-30T23:59:35","No","No","No","Internal","Noted, please repair fixture to avoid water seepage. then raise RO for new LED light with fixture."]
[null,null,null,26838,26831,"122_Sat Sep 10 2022 01:55:50 GMT+0800","2022-09-01T23:59:35","Non Conformity","Ship Staff","Ship Staff Insp.","during routine wet rounds , the fire line on deck observed to have a drop by drop leakage, further close inspection revealed that the pipe section is appreciably wasted out and is thinned down at locations. ","Deck - Pipe / Fittings","Safety / LSA / FFA","Equipment Related","","","","","new pipe readied with new sleeve, new pipe coated with protective paint coating internally. hot work concurrence seek from office and wasted out pipe section renewed. after welding , pipe section is allowed to cool down sufficiently and then pressure testing of fire line carried. found satisfactory.","2022-09-07T23:59:35","","Completed","2022-09-05T23:59:35","No","No","No","Internal"]
[null,null,null,26839,69704,"122_Thu Sep 15 2022 14:04:09 GMT+0800","2022-09-10T23:59:35","Observation","Ship Staff","Ship Staff Insp.","During AE-2 routine daily round it was observed that oil leaking from unit-3 cylinder head. ","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","AE-2 isolated and unit-3 cylinder head removed and inspected, metal gasket and V-ring on air side replaced and fitted back in place. tightened to specified hydraulic pressure . remaining units are also checked for their hydraulic pressure tightness. tappet clearances measured and adjusted. AE-2 tried out, working satisfactory and leak is rectified.","2022-10-28T23:59:35","","Completed","2022-09-11T23:59:35","No","No","No","Internal"]
[null,null,null,21156,null,"122_31/8/2021 9:05:40 pm","2022-09-28T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Mooring winch brake bands are rusted","Deck - Mooring Machinery","Mooring","Equipment Related,External Factors,Inappropriate Procedure","","","","","All mooring winch Brake band has been de-rusted completed. ","2022-12-29T23:59:35","","Completed","2022-12-13T23:59:35","No","No","No","Internal","pls update progress"]
[null,null,null,27872,70468,"122_Thu Nov 17 2022 18:18:52 GMT+0800","2022-10-28T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Provision Crane securing hook on Monkey island found corroded and damage.","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","Equipment Related","","","","","Fabricated new securing points for provision crane.","2022-11-08T23:59:35","","Completed","2022-10-29T23:59:35","No","No","No","Internal"]
[null,null,null,27873,46588,"122_Thu Nov 17 2022 18:23:10 GMT+0800","2022-11-02T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Port side accommodation ladder Bracket for placing wooden fender found damage and corroded.","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","Equipment Related","","","","","New Brackets were Fabricated and welded on Port side Gangway.","2022-11-08T23:59:35","","Completed","2022-11-05T23:59:35","No","No","No","Internal"]
[null,null,null,27874,78010,"122_Thu Nov 17 2022 18:26:07 GMT+0800","2022-11-02T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Hatch cover Inclined ladder between CH no 5 &6 bottom step found corroded and worn off.","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","Equipment Related","","","","","Bottom step was Fabricated and renewed between CH no 5 & 6.","2022-11-13T23:59:35","","Completed","2022-11-05T23:59:35","No","No","No","Internal"]
[null,null,null,27877,40456,"122_Thu Nov 17 2022 18:28:55 GMT+0800","2022-11-07T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Base of vertical ladder in CH no 5 found worn off and damage.","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","Equipment Related","","","","","Base for vertical ladder in CH no 5 was Fabricated and renewed.","2022-11-13T23:59:35","","Completed","2022-11-08T23:59:35","No","No","No","Internal"]
[null,null,null,27876,62510,"122_Tue Dec 06 2022 17:55:21 GMT+0800","2022-11-20T23:59:35","Observation","Ship Staff","Ship Staff Insp.","one fire hydrant near MAC of ER 2nd deck found leaking slightly.","E/R - Pipes/ valves & fittings,LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","Defective fire hydrant overhauled and installed. Fire line pressure tested. Found all in good order.","2022-12-13T23:59:35","","Completed","2022-11-23T23:59:35","No","No","No","Internal"]
[null,null,null,27875,48693,"122_Tue Dec 06 2022 17:53:01 GMT+0800","2022-11-26T23:59:35","Observation","Ship Staff","Ship Staff Insp.","FWG ejector pump discharge line a section of pipe found in bad condition.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Defective pipe renewed by fabricating a new pipeline. Tried out. All ok,","2022-12-13T23:59:35","","Completed","2022-11-28T23:59:35","No","No","No","Internal"]
[null,null,null,27929,93040,"122_Thu Dec 15 2022 23:18:08 GMT+0800","2022-12-01T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Junction boxes for Bunker davit port side found corroded and wasted.","Deck - Machinery","Structural Condn. / WT integrity ","Equipment Related","","","","","New Junction boxes were fabricated and welded on port side bunker davit.","2022-12-29T23:59:35","","Completed","2022-12-09T23:59:35","No","No","No","Internal"]
[null,null,null,27930,67897,"122_Wed Dec 14 2022 18:18:07 GMT+0800","2022-12-11T23:59:35","Observation","Ship Staff","Ship Staff Insp.","FWG ejector pump discharge line pipe leaky.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Leaky pipe renewed with fabricated new pipe. All ok.","2022-12-29T23:59:35","","Completed","2022-12-13T23:59:35","No","No","No","Internal"]
[null,null,null,null,46818,"122_Wed Dec 14 2022 18:29:07 GMT+0800","2022-12-11T08:00:00","Observation","Ship Staff","Ship Staff Insp.","Cooling Sea water line sections near sealing of ER 2nd Deck above feed water pumps going for consumables (accommodation AC, reefer compressor, ECR AC) are leaky. Same job already added in dock specs.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Leaky section to be monitored continuously, if leak increases, needed to change leaky section. As these pipe sections are near to sealing of ER 2nd deck, work aloft and office concurrence are required.","2023-01-29T08:00:00","","Completed","2022-12-19T08:00:00","No","No","No","Internal","Please make work plan and renew the pipe , prepare and forward work permit to office for approval. please take note, dry docking still nit fixed, it may be postponed."]
[null,null,null,null,60063,"122_Thu Nov 17 2022 16:41:54 GMT+0800","2022-09-14T08:00:00","Breakdown","Ship Staff","Ship Staff Insp.","Purifier room Exh Fan motor not operational","Critical Equip.","Safety / LSA / FFA","Equipment Related","","","","","New motor fitted in place. Trail taken found all parameters satisfactory.","2023-02-28T08:00:00","NAQU220107","Completed","2023-02-22T08:00:00","No","No","No","Internal","will supply the motor at convenient port."]
[null,null,null,null,73875,"0_Thu Nov 17 2022 16:52:09 GMT+0800","2022-10-24T08:00:00","Critical Equipment","Ship Staff","Ship Staff Insp.","Water Ingress Pre sensors of Hold#4, Hold#7 & Hold#2, Forepeak Cofferdam defective","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","Water Ingress pre sensors of hold no 2,4 & 7 and cofferdam sensor renewed. Alarm tried out working satisfactory. ","2023-03-15T08:00:00","NAQU220152, NAQU230007","Completed","2023-03-15T08:00:00","No","No","No","Internal","spare was ready at forwarder warehouse , will connect to vessel at convenient port."]
[null,null,null,null,16817,"122_Thu Jan 05 2023 15:05:30 GMT+0800","2023-01-05T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Public Addressor speaker on monkey island defective. ","Navigation - Others","Safety / LSA / FFA","Equipment Related","","","","","Spares received and speaker renewed. Working satisfactory.","2023-02-28T08:00:00","NAQU230022","Completed","2023-03-16T08:00:00","No","No","No","Internal"]
[null,null,null,null,81336,"122_Wed May 17 2023 07:15:47 GMT+0800","2023-05-16T08:00:00","Observation","Ship Staff","Ship Staff Insp.","MINOR OIL LEAKAGES FORM ALL 4 GANGWAY MOTORS ","Deck - Machinery","General Appearance","Equipment Related","","","","","SHIPYARD WILL REPAIR THE LEAKING MOTORS IN WORK SHOP. ","2023-06-30T08:00:00","","Completed","2023-06-27T08:00:00","No","No","No","Internal"]
[null,null,null,null,91169,"122_Wed May 17 2023 07:11:44 GMT+0800","2023-05-16T08:00:00","Observation","Ship Staff","Ship Staff Insp.","APT AIR VENT PIPE LEAKING IN STEERING FLAT WHEN APT OVERFLOWS.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","","","","","JOB INC. IN DD SPEC. SHOWN TO OWNER'S SUPTDT. SHIPYARD IS AWAITING APPROVAL.","2023-06-30T08:00:00","","Completed","2023-06-26T08:00:00","No","No","No","Internal"]
[null,null,null,null,99378,"122_Wed Mar 15 2023 22:08:12 GMT+0800","2023-03-15T08:00:00","Defect","Ship Staff","Ship Staff Insp."," WATER LEAKAGE FROM NO-1 TST PORT TO NO-1  CARGO HOLD.","Hull & Tanks","Cargo / Ballast Systems","Equipment Related","","","","","JOB DISCUSSED WITH SHIPYARD AND OWNER'S SUPTDT. AWAITING APPROVAL FROM OWNER'S SUPTDT.","2023-06-30T08:00:00","NA","Completed","2023-06-25T08:00:00","Yes","No","No","Internal","please inspect after cargo discharged and include work scope in DD specs for all tst tanks as necessary"]
[null,null,null,null,26901,"122_Mon Mar 06 2023 12:37:46 GMT+0800","2023-03-01T08:00:00","Defect","Ship Staff","Ship Staff Insp.","hatch cover no. 4 drive motor oil leaking through seal.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","HATCH COVER MOTOR REMOVED BY WORKSHOP FOR NECESSARY REPAIRS.","2023-06-30T08:00:00","","Completed","2023-06-24T08:00:00","No","No","No","Internal","to be rectified before departure from shipyard"]
[null,null,null,null,50225,"122_Sat Dec 31 2022 22:16:32 GMT+0800","2022-12-17T08:00:00","Defect,Observation","Ship Staff","Ship Staff Insp.","Various hydraulic line on deck are  corroded due to ageing.","Deck - Machinery,Deck - Mooring Machinery,Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","HYDRAULIC LINES WILL BE RENEWED BY THE SHIPYARD. MEASUREMENT TAKEN.","2023-06-30T08:00:00","","Completed","2023-06-30T08:00:00","No","No","No","Internal","to be rectified before vessel departure from shipyard"]
[null,null,null,null,65944,"122_Mon Sep 12 2022 17:03:40 GMT+0800","2022-09-09T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Both Fire doors on Upper Deck Entrance were found in poor condition with heavy corrosion and wastage.","Accommodation,LSA / FFA,Critical Equip.","Safety / LSA / FFA","Equipment Related","","","","","Both fire doors with frames need to be completely renewed. DD specs have been prepared in REFMAN. Awaiting supply.","2023-06-30T08:00:00","NAQU230178","Completed","2023-06-30T08:00:00","Yes","No","No","Internal","\nwill renew the door at shipyard, please advice RO number."]
[null,null,null,null,60337,"122_Mon Apr 03 2023 22:31:54 GMT+0800","2023-03-16T08:00:00","Defect","Ship Staff","Ship Staff Insp.","#1 boiler feed pump vibrates during operation , as per past history impeller is machined and fitted . suspect imbalancing as cause of vibrations.  ","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","","","","","PUMP CASING IS DAMAGED AND WAS MACHINED AND MODIFIED , PUMP ASSEMBLED AND TESTED NO VIBRATIONS.\nNEW PUMP REQUISITION IS RAISED.","2023-06-30T08:00:00","NAQU 230188 is raised for required spares","Completed","2023-07-12T08:00:00","No","No","No","Internal"]
[null,null,null,null,32191,"122_Sat Dec 31 2022 17:39:07 GMT+0800","2022-12-22T08:00:00","Defect,Observation","Ship Staff","Ship Staff Insp.","Various SW pipes in ER are with soft patches and clamps. For same job order was already in DD specs(RefMan,item#37 & #58)","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related,External Factors","","","","","ALL DEFECTIVE SEA WATER PIPELINES RENEWED IN SHIPYARD.","2023-06-30T08:00:00","","Completed","2023-06-30T08:00:00","No","No","No","Internal","to be rectified before vessel departure from shipyard"]
[null,null,null,21167,null,"122_16-09-2021 09:17:26","2022-08-10T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Stern Tube AFT seal oil content showing 0.94%. Stern tube system shows 0.04% water content.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","FWD AND AFTE SEALS RENEWED IN DRY DOCK , WHOLE SYSTEM OIL RENEWED.","2023-06-30T08:00:00","","Completed","2023-06-30T08:00:00","No","No","No","Internal","WILL RENEW BOTH SIDE OF AFT AND FWD SEAL IN DRY DOCK"]

{"sheet":"Calc","index":2,"n_rows":28,"n_cols":12,"rows_kept":28,"cut":false,"hidden":true,"merged":[]}
["Def_type","Def_cause","Equipments","VIQrefno","Observer_code"]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,"Dim itemSele As Long"]
[null,null,null,null,null,null,null,null,null,null,null,"   dim startRow as integer"]
[null,null,null,null,null,null,null,null,null,null,null,"   startRow=1"]
[null,null,null,null,null,null,null,null,null,null,null,"        For itemSele = 0 To ListBox1.ListCount - 1"]
[null,null,null,null,null,null,null,null,null,null,null,"        If ListBox1.Selected(itemSele) = True Then"]
[null,null,null,null,null,null,null,null,null,null,null,"        Worksheets(\"WorksheetName\").Range(\"A\" & startRow).Value = ListBox1.List(itemSele)"]
[null,null,null,null,null,null,null,null,null,null,null,"        startRow = startRow + 1"]
[null,null,null,null,null,null,null,null,null,null,null,"        End If"]
[null,null,null,null,null,null,null,null,null,null,null,"        Next"]
[null,null,null,null,null,null,null,null,null,null,null,"Dim LastRowA As String"]
[null,null,null,null,null,null,null,null,null,null,null,"        Dim itemSele As Long"]
[null,null,null,null,null,null,null,null,null,null,null,"       Dim startRow as integer"]
[null,null,null,null,null,null,null,null,null,null,null,"        LastRowA = ActiveSheet.Cells(Rows.count, \"A\").End(xlUp).row"]
[null,null,null,null,null,null,null,null,null,null,null,"        startQue = 0"]
[null,null,null,null,null,null,null,null,null,null,null,"        For itemSele = 0 To ListBox1.ListCount - 1"]
[null,null,null,null,null,null,null,null,null,null,null,"        For startRow = 1 To LastRowA"]
[null,null,null,null,null,null,null,null,null,null,null,"        If Worksheets(\"WorksheetName\").Range(\"A\" & startRow).Value = ListBox1.List(itemSele) Then"]
[null,null,null,null,null,null,null,null,null,null,null,"        ListBox1.Selected(itemSele) = True"]
[null,null,null,null,null,null,null,null,null,null,null,"        Exit For"]
[null,null,null,null,null,null,null,null,null,null,null,"        End If"]
[null,null,null,null,null,null,null,null,null,null,null,"        Next j"]
[null,null,null,null,null,null,null,null,null,null,null,"        Next"]
[null,null,null,null,null,null,null,null,null,null,null,"        End If"]

{"sheet":"Areaofobs","index":3,"n_rows":17,"n_cols":2,"rows_kept":17,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Cargo / Ballast Systems",11]
["Cert. & Docu.",2]
["Communication",6]
["Crew Management",3]
["Emgcy. Systems",13]
["Eng. / Strg. Comp.",14]
["General Appearance",15]
["Ice Opns.",17]
["ISM Related",7]
["ISPS Related",10]
["MARPOL Related",9]
["MLC Related",4]
["Mooring",12]
["Navigation",5]
["Safety / LSA / FFA",8]
["Structural Condn. / WT integrity ",16]

{"sheet":"Vessel_type","index":4,"n_rows":1,"n_cols":2,"rows_kept":1,"cut":false,"hidden":true,"merged":[]}
["Vessel_type","ID"]

{"sheet":"Deficiency_type","index":5,"n_rows":8,"n_cols":3,"rows_kept":8,"cut":false,"hidden":true,"merged":[]}
["TITLE","Type of deficiency_description","ID"]
["Breakdown",null,6]
["Critical Equipment",null,4]
["Defect",null,1]
["Guarantee Claim",null,8]
["Non Conformity",null,2]
["Observation",null,3]
["Other",null,7]

{"sheet":"VIQrefno","index":6,"n_rows":1,"n_cols":3,"rows_kept":1,"cut":false,"hidden":true,"merged":[]}
["VIQ_ref_no","Risk Value of observation","ID"]

{"sheet":"Equipment_list","index":7,"n_rows":28,"n_cols":3,"rows_kept":28,"cut":false,"hidden":true,"merged":[]}
["TITLE","Equipment_list_description","ID"]
["Accommodation",null,12]
["Cargo Mach.",null,13]
["Critical Equip.",null,16]
["Deck - Machinery",null,18]
["Deck - Mooring Machinery",null,15]
["Deck - Pipe / Fittings",null,20]
["Documentation",null,21]
["E/R - Air Comp.",null,8]
["E/R - Aux. Engine",null,4]
["E/R - Aux. Mach.",null,7]
["E/R - Boiler",null,5]
["E/R - Main Engine",null,3]
["E/R - Pipes/ valves & fittings",null,9]
["E/R - Pumps",null,32]
["E/R - Purifier",null,6]
["Elect. Mach. & Equip.",null,10]
["Hull & Tanks",null,19]
["Inert Gas",null,14]
["LSA / FFA",null,17]
["Miscellaneous",null,22]
["Navigation - DGPS / EPFS / AIS",null,28]
["Navigation - ECDIS",null,25]
["Navigation - Echo Sounder / Speed Log",null,26]
["Navigation - GMDSS & Communication",null,23]
["Navigation - Others",null,11]
["Navigation - RADAR",null,24]
["Navigation - VDR / BNWAS",null,30]

{"sheet":"PSC_MOU","index":8,"n_rows":11,"n_cols":3,"rows_kept":11,"cut":false,"hidden":true,"merged":[]}
["TITLE","PSC_MOU_description","ID"]
["Asia and the Pacific",null,2]
["Caribbean",null,4]
["Europe and the North Atlantic",null,1]
["Latin America",null,3]
["The Black Sea region",null,6]
["The Indian Ocean",null,8]
["The Mediterranean",null,7]
["The Riyadh MoU",null,9]
["USCG",null,10]
["West and Central Africa",null,5]

{"sheet":"Inspection_type","index":9,"n_rows":13,"n_cols":2,"rows_kept":13,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Bunkering Audit",14]
["Cargo Audit",17]
["Engineering Audit",16]
["ISM Audit",2]
["ISPS Audit",3]
["IT Audit",10]
["MLC Audit",1]
["Mooring Audit",9]
["Nav Audit / Verification",8]
["Onboard Training",18]
["Ship Staff Insp.",15]
["Suptd. Insp.",13]

{"sheet":"Deficiency_Cause","index":10,"n_rows":8,"n_cols":3,"rows_kept":8,"cut":false,"hidden":true,"merged":[]}
["TITLE","Deficiency_Cause_description","ID"]
["Behaviour Based",null,1]
["Equipment Related",null,4]
["External Factors",null,5]
["Human Error",null,7]
["Inappropriate Procedure",null,8]
["Industry Issue",null,6]
["Knowledge Based",null,3]

{"sheet":"Observer_code","index":11,"n_rows":3,"n_cols":3,"rows_kept":3,"cut":false,"hidden":true,"merged":[]}
["TITLE","Observer_code_description","ID"]
["Owner / Marine / Tech. Suptd.",null,3]
["Ship Staff",null,2]

{"sheet":"Status_code","index":12,"n_rows":6,"n_cols":3,"rows_kept":6,"cut":false,"hidden":true,"merged":[]}
["TITLE","Status_code_description","ID"]
["Completed",null,6]
["Deferred to D D",null,5]
["In progress",null,3]
["Not Started",null,2]
["Waiting spare",null,4]

{"sheet":"PSC_ref_no","index":13,"n_rows":19,"n_cols":2,"rows_kept":19,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Alarms",9]
["Cargo operations including equipment",7]
["Certificates & Documentation",2]
["Dangerous Goods",13]
["Emergency Systems",5]
["Fire safety",8]
["ISM",16]
["ISPS",17]
["Life saving appliances",12]
["MLC, 2006",18]
["Other",19]
["Pollution Prevention",15]
["Propulsion and auxiliary machinery",14]
["Radio communication",6]
["Safety of Navigation",11]
["Structural condition",3]
["Water/Weathertight condition",4]
["Working and Living Conditions",10]

{"sheet":"Risk_value_of_obs","index":14,"n_rows":1,"n_cols":2,"rows_kept":1,"cut":false,"hidden":true,"merged":[]}
["Risk Value of observation","ID"]

{"sheet":"Year","index":15,"n_rows":18,"n_cols":1,"rows_kept":18,"cut":false,"hidden":true,"merged":[]}
["Year"]
[2014]
[2015]
[2016]
[2017]
[2018]
[2019]
[2020]
[2021]
[2022]
[2023]
[2024]
[2025]
[2026]
[2027]
[2028]
[2029]
[2030]

{"sheet":"Month","index":16,"n_rows":13,"n_cols":1,"rows_kept":13,"cut":false,"hidden":true,"merged":[]}
["Month"]
["Jan"]
["Feb"]
["Mar"]
["Apr"]
["May"]
["Jun"]
["Jul"]
["Aug"]
["Sep"]
["Oct"]
["Nov"]
["Dec"]

{"sheet":"Date_","index":17,"n_rows":32,"n_cols":1,"rows_kept":32,"cut":false,"hidden":true,"merged":[]}
["Date"]
["01"]
["02"]
["03"]
["04"]
["05"]
["06"]
["07"]
["08"]
["09"]
[10]
[11]
[12]
[13]
[14]
[15]
[16]
[17]
[18]
[19]
[20]
[21]
[22]
[23]
[24]
[25]
[26]
[27]
[28]
[29]
[30]
[31]

{"sheet":"Sheet1","index":18,"n_rows":24,"n_cols":6,"rows_kept":24,"cut":false,"hidden":true,"merged":[]}
[]
[null,"ID","E",null,"Date Recorded",1]
[null,"UNIQUE ID","F",null,"Type of Deficiency",2]
[1,"Date Recorded","G",null,"Observer code",3]
["ignore","Vessel Type","H",null,"Type of Inspection",4]
[null,"Internal / External","I",null,"Description of Deficiency",5]
[null,"Drydock","J",null,"Equipment Categories",6]
[null,"Information Sharing","K",null,"Area of Observation",7]
[null,"Critical_item","L",null,"Deficiency Cause",8]
[null,"Deficiency Type","M",null,"VIQ Ref Number",9]
[null,"Deficiency Cause","N",null,"Risk Value of Obs",10]
[null,"Inspection Type","O",null,"PSC Ref Number",11]
[null,"Equipments","P",null,"PSC MOU ID",12]
[null,"VIQ Reference Number","Q",null,"Action Taken or Required",13]
[null,"Risk Value of the observation","R",null,"Target Date",14]
[null,"PSC Reference Number","S",null,"PO Ref No.",15]
[null,"PSC MOU","T",null,"Status Code",16]
[null,"Observer Code","U",null,"Date Completed",17]
[null,"Target Date","V",null,"Drydock",18]
[null,"Status Code","W",null,"Info Sharing",19]
[null,"Description of Deficiency","X",null,"Critical Item Flag",20]
[null,"Action taken / required","Y",null,"Audit Type",21]
[null,"PO ref no","Z"]
[null,"Date completed","AA"]

{"sheet":"Ship_information","index":19,"n_rows":2,"n_cols":3,"rows_kept":2,"cut":false,"hidden":true,"merged":[]}
["Ship_ID","Ship_Name","FILE_NAME"]
["122","AQUAHOLIC (19-12-2022)","122_1671428759825.xlsm"]

{"sheet":"External_Deficiency_type","index":20,"n_rows":5,"n_cols":3,"rows_kept":5,"cut":false,"hidden":true,"merged":[]}
["TITLE","Type of deficiency_description","ID"]
["Condn of Class / Memo",null,5]
["Defect",null,1]
["Non Conformity",null,2]
["Observation",null,3]

{"sheet":"External_Inspection_type","index":21,"n_rows":11,"n_cols":2,"rows_kept":11,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Cargo Audit",17]
["Flag State Insp.",5]
["ISM Audit",2]
["ISPS Audit",3]
["MLC Audit",1]
["Nav Audit / Verification",8]
["OM Insp. (Eg. SIRE / CDI etc.)",6]
["Others (Eg. Insurance etc.)",12]
["PSC Inspection",4]
["Terminal Insp.",11]

{"sheet":"External_Observer_code","index":22,"n_rows":7,"n_cols":3,"rows_kept":7,"cut":false,"hidden":true,"merged":[]}
["TITLE","Observer_code_description","ID"]
["Class Surveyor",null,4]
["FSC Inspector",null,5]
["Others (Eg. Insurance etc.)",null,9]
["PSC Insp.",null,6]
["SIRE / CDI Insp.",null,8]
["Terminal Insp.",null,7]

{"sheet":"Sheet Version","index":23,"n_rows":2,"n_cols":2,"rows_kept":2,"cut":false,"hidden":true,"merged":[]}
["Version","Title"]
["2.0","Version 2.0"]