{"text_format":"1","workbook":"xlsx","n_sheets":24,"sheets":["Mainsheet","Completed","Calc","Areaofobs","Vessel_type","Deficiency_type","VIQrefno","Equipment_list","PSC_MOU","Inspection_type","Deficiency_Cause","Observer_code","Status_code","PSC_ref_no","Risk_value_of_obs","Year","Month","Date_","Sheet1","Ship_information","External_Deficiency_type","External_Inspection_type","External_Observer_code","Sheet Version"],"not_rendered":{"charts":0,"images":1,"macros":1,"external_links":0,"defined_names":12,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Mainsheet","index":0,"n_rows":22,"n_cols":28,"rows_kept":22,"cut":false,"hidden":false,"merged":[[10,8,10,9],[10,12,10,13],[12,6,12,27],[8,6,8,27]]}
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,"Defect - Damage Monitoring Sheet"]
[]
[null,null,null,null,null,null,null,"Date of Report","01-Sep-2023",null,null,"Ship Name","ANTWERP (19-08-2023)"]
[]
[null,null,null,null,null,null,"VERSION : 2.0"]
[]
[]
[]
[null,null,null,"ID","SHIPSIDE UNIQUEID","UNIQUE ID","Date Recorded","Type of Deficiency","Observer code","Type of Inspection","Description of Deficiency","Equipment Categories","Area of Observation","Deficiency Cause","VIQ Ref Number","Risk Value of Obs","PSC Ref Number","PSC MOU ID","Action Taken or Required","Target Date","PO Ref No.","Status Code","Date Completed","Drydock","Info Sharing","Critical Item","Audit Type","Superintendent Remarks"]
[null,null,null,31156,58302,"107_Wed Aug 09 2023 14:27:27 GMT+0800","2023-07-24T23:59:35","Observation","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","The hatch coaming (internal) plates and lower stool plates of nine (9) cargo holds were noted with loosened rust scale covering.","Miscellaneous","Cargo / Ballast Systems","External Factors","","","","","","2023-11-24T23:59:35","","Not Started",null,"No","No","No","External"]
[null,null,null,31020,54354,"107_Tue Aug 01 2023 17:41:53 GMT+0800","2023-07-30T23:59:35","Other","Others (Eg. Insurance etc.)","Nav Audit / Verification","RADAR JMA 9303 IMAGE QUALITY  IS POOR, \nNRG-88, TR CONTROL: CMG-898 AND PM UNIT: NJU-63 REPLACEMENT RECOMMENDED BY RADAR TECHNICIAN","Navigation - DGPS / EPFS / AIS","Navigation","Equipment Related","","","","","REPLACEMENT OF PM AT NEXT CONVENIENT PORT","2023-10-31T23:59:35","","Not Started",null,"No","No","No","Internal"]
[null,null,null,31181,32198,"107_Thu Aug 17 2023 18:24:55 GMT+0800","2023-08-16T23:59:35","Defect","Ship Staff","Ship Staff Insp.","The ROS1 of Alarm Monitoring System is activating the DPU fail alarms due to communication error. ","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","The service engineer attended and advised to upgrade the System","2023-11-16T23:59:35","ANTW235007","Waiting spare",null,"No","No","No","Internal"]
[null,null,null,31182,96408,"107_Thu Aug 17 2023 18:37:24 GMT+0800","2023-08-16T23:59:35","Defect","Ship Staff","Ship Staff Insp.","The NO.1 boiler feed water pump is not developing sufficient pressure. ","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","Pump overhauled and inspected. Found middle casing vanes are eroded. Need to renew the middle casing. Waiting spare.","2023-11-16T23:59:35","ANTW230251","Waiting spare",null,"No","No","No","Internal"]
[null,null,null,null,70739,"107_Thu Aug 31 2023 17:21:55 GMT+0800","2023-08-16T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Lifeboat Davit limit switch found corroded and sluggish in operation during lifeboat lowering.","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","Limit switch eased up, now working satisfactory. Spare RO ANTW230256  raised.","2023-11-15T08:00:00","","Waiting spare",null,"No","No","No","Internal"]

{"sheet":"Completed","index":1,"n_rows":272,"n_cols":28,"rows_kept":272,"cut":false,"hidden":false,"merged":[[10,8,10,9],[10,12,10,13],[12,6,12,27],[8,6,8,27]]}
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,"Defect - Damage Monitoring Sheet"]
[]
[null,null,null,null,null,null,null,"Date of Report","01-Sep-2023",null,null,"Ship Name","ANTWERP (19-08-2023)"]
[]
[null,null,null,null,null,null,"VERSION : 2.0"]
[]
[]
[]
[null,null,null,"ID","SHIPSIDE UNIQUEID","UNIQUE ID","Date Recorded","Type of Deficiency","Observer code","Type of Inspection","Description of Deficiency","Equipment Categories","Area of Observation","Deficiency Cause","VIQ Ref Number","Risk Value of Obs","PSC Ref Number","PSC MOU ID","Action Taken or Required","Target Date","PO Ref No.","Status Code","Date Completed","Drydock","Info Sharing","Critical Item","Audit Type","Superintendent Remarks"]
[null,null,null,28245,null,"107_Tue Jan 10 2023 06:17:41 GMT+0000",null,"Observation","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","","Inert Gas,Deck - Pipe / Fittings,E/R - Pipes/ valves & fittings","","Behaviour Based,Equipment Related,External Factors","","","","","",null,"","Completed",null,"No","No","No","External"]
[null,null,null,14664,null,"107_Mon Nov 16 2020 10:52:14 GMT+0000","2020-01-11T23:59:35","Observation","Ship Staff","Ship Staff Insp.","VDR display shows radar alert alarm sometimes.","Navigation - VDR / BNWAS","Communication","Equipment Related","","","","","already completed ","2020-12-14T23:59:35","","Completed","2020-01-11T23:59:35","No","No","No","Internal","Pls do check and find out the cause of alarms on the VDR display  monitor"]
[null,null,null,14673,null,"107_Mon Nov 16 2020 11:11:18 GMT+0000","2020-01-11T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Port side windlass brake lining  required renewal","Deck - Mooring Machinery","General Appearance","Equipment Related","","","","","REPLACE BY DD","2021-06-03T23:59:35","ANTW200013","Completed","2021-09-04T23:59:35","Yes","No","No","Internal","please update status due to docking under extend to Sep 2021"]
[null,null,null,15571,null,"107_Tue Dec 08 2020 10:36:12 GMT+0000","2020-03-02T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Funnel painting faded, same to be painted with designated LOGO.","Deck - Pipe / Fittings","General Appearance","External Factors","","","","","Completed forward, portside & stbdside painting jobs.behind side will be complete when D-Docking.","2021-05-31T23:59:35","","Completed","2021-06-22T23:59:35","No","No","No","Internal","will do it during docking under extend to Sep 2021"]
[null,null,null,15566,null,"107_Tue Dec 08 2020 08:23:49 GMT+0000","2020-03-16T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Port Windlass: Outer drum bush is badly worn – requires to be renewed soonest to avoid shaft damage. Main shaft bearing is badly worn out which causing excessive shaft movement.","Deck - Mooring Machinery","Mooring","Equipment Related","","","","","oVERHAULED IN DRY DOCK","2021-06-08T23:59:35","","Completed","2021-09-08T23:59:35","Yes","No","No","Internal","Pls  check spare R.O.B  and submit R.O. for the spare parts if require."]
[null,null,null,14666,null,"107_Mon Nov 16 2020 10:56:19 GMT+0000","2020-11-15T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Main engine Alpha lub station pump no.1 pipe connection leaking","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Try one more to retighten again, no leaking now","2021-01-30T23:59:35","","Completed","2021-01-29T23:59:35","No","No","No","Internal","Pls  do rectify as soon as possible."]
[null,null,null,14670,null,"107_Mon Nov 16 2020 11:04:36 GMT+0000","2020-11-15T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Steering gear no. 1& 2 hyd pump oil seal  found leaking excessively","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Shore service engineers on board for repair @ Sgp 2020-11-27~30. Now new problem are leaking from shaft seal of rudder angle. So suugest to close this & writen new.","2020-12-30T23:59:35","ANTW205043","Completed","2020-11-29T23:59:35","No","No","No","Internal","Pls submit requisition for spare parts"]
[null,null,null,14675,null,"107_Mon Nov 16 2020 11:14:20 GMT+0000","2020-11-15T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Hatch covers hydraulic pipes corroded and leaking in various locations, required renewal and press test","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","","","","","Some pipe renewed by crew already.","2020-12-29T23:59:35","","Completed","2020-12-02T23:59:35","No","No","No","Internal","Leaky pipes renewed. Pls  submit RO of the  required pipes & fittings ."]
[null,null,null,14676,null,"107_Mon Nov 16 2020 11:15:46 GMT+0000","2020-11-15T23:59:35","Defect","Ship Staff","Ship Staff Insp.","ME Lub oil purifier supply pump  are  not working","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","","","","","Electrical power supply issue was solved and made operational. ","2021-09-03T23:59:35","ANTW-007-2021","Completed","2021-09-08T23:59:35","No","No","No","Internal","Pls do check and plan to overhaul pump if required."]
[null,null,null,14677,null,"107_Mon Nov 16 2020 11:18:05 GMT+0000","2020-11-15T23:59:35","Defect","Ship Staff","Ship Staff Insp.","M/E lube oil stand by  pump  found starting auto but no alert alarm activated in ECR panel","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","\"cyclect\" engineers on board for check, test, later supplied 3+7pcs contactor & renewed by crew. Test & found normal, but found some problem after sail again. So closed this & writen other later.","2021-01-14T23:59:35","ANWT205042, 205054.","Completed","2020-11-28T23:59:35","No","No","No","Internal","Pls advise which pump contactor are having problem now."]
[null,null,null,14678,null,"107_Mon Nov 16 2020 11:19:28 GMT+0000","2020-11-15T23:59:35","Defect","Ship Staff","Ship Staff Insp.","M/E JCFW  stand by  pump  found starting auto but no alert alarm activated in ECR panel","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","","","","","Same than ME LO pump","2021-01-14T23:59:35","ANWT205042, 205054","Completed","2020-11-28T23:59:35","No","No","No","Internal","Pls  renew contactor after receiving spare."]
[null,null,null,14679,null,"107_Mon Nov 16 2020 11:20:54 GMT+0000","2020-11-15T23:59:35","Defect,Observation","Ship Staff","Ship Staff Insp.","Provision crane hydraulic piping  condition not good, required renewal","Deck - Machinery","Eng. / Strg. Comp.","Equipment Related","","","","","Renewed many soft hose by workshop personal & some can't renewed due to old connector welding by previous crew. these hose stay on board for spare.","2021-06-03T23:59:35","ANTW205043","Completed","2021-09-06T23:59:35","No","No","No","Internal","Pls renew if spare pipe available or submit requisition."]
[null,null,null,14680,null,"107_Mon Nov 16 2020 11:22:28 GMT+0000","2020-11-15T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Hypermist HP pump press gauge  is not working","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","The spare come on board,We intalled finish.Now is good.","2021-02-27T23:59:35","ANTW 205078","Completed","2021-01-28T23:59:35","No","No","No","Internal","Pls order new press gauge if not available onboard."]
[null,null,null,14681,null,"107_Mon Nov 16 2020 11:24:05 GMT+0000","2020-11-15T23:59:35","Other","Ship Staff","Ship Staff Insp.","There was no ODS & Suphur content record book found on board","Documentation","Cert. & Docu.","Equipment Related","","","","","SI bring 2books - Bunker sample & SECA FCO record book on board 20-Nov-2020 ( Incluclinding S%). Re ODS office have standard \"word\" file.","2020-12-15T23:59:35","","Completed","2020-11-29T23:59:35","No","No","No","Internal",""]
[null,null,null,14682,null,"107_Mon Nov 16 2020 11:25:29 GMT+0000","2020-11-15T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Aux boiler feed water automatic  control valve  not working","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Crew adjusted already. Service on board when call SIN 27-Nov also.","2020-12-15T23:59:35","ANTW205033","Completed","2020-11-28T23:59:35","No","No","No","Internal","Automatic control feed valve function  tried out during boiler health check by  service technicians."]
[null,null,null,14683,null,"107_Mon Nov 16 2020 11:26:38 GMT+0000","2020-11-15T23:59:35","Defect","Ship Staff","Ship Staff Insp.","A/E & M/E FO  back wash  filters are  leaking thru the gland","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Retighten the connecting flanges after dismantled the Viscosity units..","2020-12-30T23:59:35","","Completed","2020-12-04T23:59:35","No","No","No","Internal","Pls submit R.O. for necessary repair kits."]
[null,null,null,15233,null,"107_Wed Nov 25 2020 05:49:34 GMT+0000","2020-11-24T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Exhaust Gas Economizer soot blower two sets valves  are seized, require to be made operational.","E/R - Boiler,E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","External Factors","","","","","Action taken","2020-12-14T23:59:35","","Completed","2020-11-30T23:59:35","No","No","No","Internal","Faulty soot blower (aft ) dismantled, overhauled and fitted back. by shore technicians at Singapore. Tried out found satisfactory."]
[null,null,null,15234,null,"107_Wed Nov 25 2020 05:52:02 GMT+0000","2020-11-24T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Oily Water Separator 15 ppm alarm and Three way valves functioning to be checked. OWS damage pipes to be renewed.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Action  taken","2020-12-09T23:59:35","","Completed","2020-11-29T23:59:35","No","No","No","Internal","15 ppm OCM renewed and 3-way valve function tested along with the alarms. found satisfactory.  Damage pipes renewed."]
[null,null,null,15235,null,"107_Wed Nov 25 2020 05:53:40 GMT+0000","2020-11-24T23:59:35","Defect","Ship Staff","Ship Staff Insp.","HFO Purifier  No. 1 and  M/E L.O. purifier are not working","E/R - Purifier","Eng. / Strg. Comp.","Equipment Related","","","","","Action Taken","2020-12-09T23:59:35","","Completed","2020-11-29T23:59:35","No","No","No","Internal","HFO purifier No.1 and ME L.O. purifier   health check carried out  and  tried out satisfactorily by shore technician at singapore."]
[null,null,null,15236,null,"107_Wed Nov 25 2020 05:55:41 GMT+0000","2020-11-24T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Aux boiler combustion control system health check required to be carried out","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","Action  Taken","2020-12-09T23:59:35","","Completed","2020-11-29T23:59:35","No","No","No","Internal","Aux Boiler combustion control system health checks carried out at  Singapore this time by shore technicians."]
[null,null,null,15238,null,"107_Wed Nov 25 2020 05:59:27 GMT+0000","2020-11-24T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Incinerator failed to fire with Waste oil","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Action Taken","2020-12-09T23:59:35","","Completed","2020-11-29T23:59:35","No","No","No","Internal","Trouble shooting carried out and Waste oil pump overhauled, tried out-found satisfactory."]
[null,null,null,15239,null,"107_Wed Nov 25 2020 06:01:46 GMT+0000","2020-11-24T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Accommodation A/C compressor required to be overhaul as no record from previous owners","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","Job attended by Breeze in DD, problem was with one expansion valve, same replaced, compressor is in order","2021-04-05T23:59:35","ANTW 205045 rcvd on board @ 20201129SIN.","Completed","2021-04-08T23:59:35","Yes","No","No","Internal","To overhaul the compressor during DD."]
[null,null,null,15240,null,"107_Wed Nov 25 2020 06:04:23 GMT+0000","2020-11-24T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Aux engine no. 1 &  2 running hours counter not working","Elect. Mach. & Equip.","Eng. / Strg. Comp.","External Factors","","","","","Rectified in Dry Dock","2021-06-03T23:59:35","ANTW 205079","Completed","2021-09-08T23:59:35","No","No","No","Internal","will supply in next convenient port"]
[null,null,null,15243,null,"107_Wed Nov 25 2020 06:11:18 GMT+0000","2020-11-24T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Ballast control  system   04 nos valves are show error from cargo control room","Deck - Pipe / Fittings","Eng. / Strg. Comp.","Equipment Related","","","","","The spare was  supply on S.G.P .Ballast control system 2 sets valve renewed.Now all valve show( indictor) is normal.","2021-05-30T23:59:35","Exchanged by ANTW215053.","Completed","2021-05-17T23:59:35","No","No","No","Internal","Service technicians attended at Singapore. Pls test the valves operation and advise."]
[null,null,null,15244,null,"107_Wed Nov 25 2020 06:13:48 GMT+0000","2020-11-24T23:59:35","Defect","Ship Staff","Ship Staff Insp.","VDR and Navigation equipment health check to be carried out.","Elect. Mach. & Equip.,Navigation - VDR / BNWAS","Communication","Equipment Related","","","","","Action Taken","2020-12-09T23:59:35","","Completed","2020-11-29T23:59:35","No","No","No","Internal","VDR and Navigation equipment's health check carried out  by Service technician  at  Singapore this time."]
[null,null,null,15245,null,"107_Wed Nov 25 2020 06:15:41 GMT+0000","2020-11-24T23:59:35","Defect","Ship Staff","Ship Staff Insp.","VSAT antenna upgrading to be carried out","Navigation - Others","Navigation","Equipment Related","","","","","Action Taken","2020-12-09T23:59:35","","Completed","2020-11-29T23:59:35","No","No","No","Internal","Service technician attended in Singapore and VSAT antenna upgraded."]
[null,null,null,15246,null,"107_Wed Nov 25 2020 06:18:02 GMT+0000","2020-11-24T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Elevator annual servicing to be carried out","Elect. Mach. & Equip.","Safety / LSA / FFA","Equipment Related","","","","","Action Taken","2020-12-09T23:59:35","","Completed","2020-11-29T23:59:35","No","No","No","Internal","Service technician attended in Singapore and annual servicing completed ."]
[null,null,null,15247,null,"107_Wed Nov 25 2020 06:20:42 GMT+0000","2020-11-24T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Life rafts  annual servicing to be carried out","LSA / FFA","Safety / LSA / FFA","Behaviour Based","","","","","Action Taken","2020-12-09T23:59:35","","Completed","2020-11-29T23:59:35","No","No","No","Internal","All life rafts are renewed with new types  this time at Singapore."]
[null,null,null,15248,null,"107_Wed Nov 25 2020 06:22:49 GMT+0000","2020-11-24T23:59:35","Observation","Ship Staff","Ship Staff Insp.","VSAT & ECDIS cable laying to be carried out","Navigation - ECDIS","Navigation","Equipment Related","","","","","Action Taken","2020-12-09T23:59:35","","Completed","2020-11-29T23:59:35","No","No","No","Internal","Cable laid  up  during her stay in Singapore."]
[null,null,null,15249,null,"107_Wed Nov 25 2020 06:24:52 GMT+0000","2020-11-24T23:59:35","Observation","Ship Staff","Ship Staff Insp.","2nd ECDIS maker FURUNO to be installed  based on owner approval","Navigation - ECDIS","Navigation","Equipment Related","","","","","Action  Taken","2020-12-09T23:59:35","","Completed","2020-11-29T23:59:35","No","No","No","Internal","2nd ECDIS installed on board , Maker: FURUNO, tried out found satisfactory."]
[null,null,null,15250,null,"107_Wed Nov 25 2020 06:48:26 GMT+0000","2020-11-24T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Ship Staff Insp.","General inspection and cleaning  of Hull,  flat bottom, vertical side, sea chest, rudder & Propeller","Hull & Tanks","Structural Condn. / WT integrity ","External Factors","","","","","Action Taken","2020-11-29T23:59:35","","Completed","2020-11-28T23:59:35","No","No","No","Internal","Diving company from Big M Marine  Pte Ltd, Singapore  inspected and cleaned up Hull, flat bottom, vertical side, sea chest  , rudder and Propeller.  propeller polished."]
[null,null,null,15550,null,"107_Tue Dec 08 2020 05:52:01 GMT+0000","2020-11-26T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","New KVH antenna installation:\nNew antenna and pedestal is installed at Singapore.\nDistance piece and pedestal to be \tpainted soonest prior stars rusting. Apply primer and final coat.","Navigation - GMDSS & Communication","Navigation","External Factors","","","","","completed","2020-12-20T23:59:35","","Completed","2020-12-02T23:59:35","No","No","No","Internal","Distance piece and pedestal to be \tpainted soonest prior stars rusting. Apply primer and final coat."]
[null,null,null,15551,null,"107_Tue Dec 08 2020 05:55:15 GMT+0000","2020-11-26T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Low insulation alarm (Earthing) on Main switch board and  Emergency Switchboard.\n\nFor 110 volts feeder panel observed low insulation on main switch board and emergency switchboard.\nETO need to resolve and clear the low insulation alarm for 110 volts line. It \tshould be close to infinite.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","External Factors","","","","","Some galley equipments no good, repaired.","2020-12-20T23:59:35","","Completed","2020-12-07T23:59:35","No","No","No","Internal","Pls do check the source of low insulation and rectify."]
[null,null,null,15552,null,"107_Tue Dec 08 2020 05:57:41 GMT+0000","2020-11-26T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","VDR float free (EPIRB) capsule: VDR Float free capsule junction box which is located on aft side of the bridge, bracket is corroded and junction box is just hanging with two bolts.\nNew holding plate to be fitted, apply paint then fit float free EPIRB junction \tbox properly.","Deck - Pipe / Fittings","Navigation","External Factors","","","","","make new bracket and maintannace attention","2020-12-30T23:59:35","","Completed","2020-11-11T23:59:35","No","No","No","Internal","New holding plate to be fitted, apply paint then fit float free EPIRB junction \tbox properly."]
[null,null,null,15553,null,"107_Tue Dec 08 2020 06:00:21 GMT+0000","2020-11-26T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Old MF/HF ATU unit: Old MF/HF ATU (Antenna coupler) unit is still in place. This is not in use. Remove old ATU unit and dispose.","Elect. Mach. & Equip.","Navigation","External Factors","","","","","completed","2021-12-08T23:59:35","","Completed","2020-12-08T23:59:35","No","No","No","Internal","Pls Remove old ATU unit and dispose."]
[null,null,null,15554,null,"107_Tue Dec 08 2020 06:02:53 GMT+0000","2020-11-26T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Present MF/HF ATU Unit (On compass deck): New MF/HF ATU unit base plate is corroded and rusted. \nRemove the ATU unit, chip and paint the base plate and fit back the ATU \tunit. Also make sure grounding copper strip is properly fitted to hull and ATU.","Elect. Mach. & Equip.","Navigation","External Factors","","","","","completed","2020-12-30T23:59:35","","Completed","2020-12-04T23:59:35","No","No","No","Internal","Remove the ATU unit, chip and paint the base plate and fit back the ATU \tunit. Also make sure grounding copper strip is properly fitted to hull and ATU."]
[null,null,null,15555,null,"107_Tue Dec 08 2020 06:06:02 GMT+0000","2020-11-26T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","New Wartsila / Transas SSAS and Tracking system: Refer below photos. ETO has put the ON/OFF switch, this switch actually not \trequire as main battery charger has fuses inside. If it is connected with other equipment then need to secure this switch and DC power cable properly to avoid short circuit in future.","Elect. Mach. & Equip.","General Appearance","External Factors","","","","","completed","2020-12-30T23:59:35","","Completed","2020-12-04T23:59:35","No","No","No","Internal","If  ON/OFF switch  is  not connected with other \tequipment then need to secure this switch and DC power cable properly to \tavoid short circuit in future."]
[null,null,null,15556,null,"107_Tue Dec 08 2020 06:08:35 GMT+0000","2020-11-26T23:59:35","Observation","Ship Staff","Suptd. Insp.","Wi-Fi unit for officer’s recreation room: New LAN cable to be laid from CCR (Chief officer desk) ships network switch till Officer’s recreation room.\nOnce LAN cable is laid and RJ-45 sockets are fitted then shift the Wi-Fi unit \tpresently fitted on D-Deck to Officer’s re-creation room. \nAs per company policy Wi-Fi should be in the Crew and Officer’s re-creation rooms.","Elect. Mach. & Equip.","General Appearance","External Factors","","","","","completed","2020-12-30T23:59:35","","Completed","2020-12-07T23:59:35","No","No","No","Internal","Once LAN cable is laid and RJ-45 sockets are fitted then shift the Wi-Fi unit \tpresently fitted on D-Deck to Officer’s re-creation room."]
[null,null,null,15558,null,"107_Tue Dec 08 2020 07:43:47 GMT+0000","2020-11-27T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Ship Staff Insp.","Deck hydraulic pipes for hatch cover corroded in various places, all pipes to be press tested and leaky pipes to be renewed.","Deck - Pipe / Fittings","General Appearance","External Factors","","","","","All wasted/corroded Hydraulic line on deck replaced with new pipes in DD","2021-05-29T23:59:35","ANWT210015.","Completed","2021-03-08T23:59:35","Yes","No","No","Internal","keep upgrading to bring up vessel performance"]
[null,null,null,15560,null,"107_Tue Dec 08 2020 07:47:07 GMT+0000","2020-11-27T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Engine room supply fan suction nets heavily rusted, same to be de-rusted and painted.","Elect. Mach. & Equip.","General Appearance","External Factors","","","","","Supply fan suction to be de-rusted and painted","2021-01-30T23:59:35","","Completed","2021-01-02T23:59:35","No","No","No","Internal"]
[null,null,null,15564,null,"107_Tue Dec 08 2020 08:17:57 GMT+0000","2020-11-27T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Domestic fridge compressor no. 1 sighted oil level too low and oil charged, same oil separator required to be checked and oil low level alarm to be tested for both the compressors.","E/R - Aux. Mach.","Eng. / Strg. Comp.","External Factors","","","","","Refri.oil top-up, & check, no found any leaking.","2020-12-30T23:59:35","","Completed","2020-12-04T23:59:35","No","No","No","Internal","Pls check the condition of the oil separator and and oil low level alarm to be tested for both the compressors."]
[null,null,null,15561,null,"107_Tue Dec 08 2020 07:49:14 GMT+0000","2020-11-28T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","M/E F.O. viscosity meter assy removed by UNIMARINE and off landed at Singapore for repair.","E/R - Pumps","Eng. / Strg. Comp.","External Factors","","","","","M/E F.O viscosity controller intalled finish.Test not leaking, Now the viscosity controller working at visc control model already.","2021-01-30T23:59:35","","Completed","2021-02-22T23:59:35","No","No","No","Internal","Viscosity controller pump unit overhauled  at Singapore and  received  vessel At Fujairah on 28 Jan 2021. Pls fit back & try out."]
[null,null,null,15563,null,"107_Tue Dec 08 2020 07:53:10 GMT+0000","2020-11-28T23:59:35","Defect","Ship Staff","Ship Staff Insp.","No #1  Boiler supply pump  dish press low, new spare pump will be required to supply","E/R - Pumps","Eng. / Strg. Comp.","External Factors","","","","","The completed new pump & motor refitted on position by workshop, test & found ok. Old pump for spare also.","2020-12-30T23:59:35","ANTW205058","Completed","2020-11-28T23:59:35","No","No","No","Internal","New pump sourcing in progress."]
[null,null,null,15570,null,"107_Tue Dec 08 2020 10:34:31 GMT+0000","2020-11-28T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Ship Staff Insp.","Port & Stbd bunker station pipes drain lines sighted corroded, same to de-rusted and painted.","Deck - Pipe / Fittings","General Appearance","External Factors","","","","","MAINTENANCE PLAN IN PROGRESS","2021-01-30T23:59:35","","Completed","2020-12-12T23:59:35","No","No","No","Internal"]
[null,null,null,15572,null,"107_Tue Dec 08 2020 10:38:01 GMT+0000","2020-11-28T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Ship Staff Insp.","Lifeboat davit (P&S) gearbox motor housing corroded, same to be de-rusted and painted.","Deck - Pipe / Fittings","General Appearance","External Factors","","","","","Completed de-rusted and painted @ 20201212.","2020-12-30T23:59:35","","Completed","2020-12-11T23:59:35","No","No","No","Internal"]
[null,null,null,15573,null,"107_Tue Dec 08 2020 10:39:34 GMT+0000","2020-11-28T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Emergency generator room top deck all empty drums to be removed and deck to be painted.","Miscellaneous","General Appearance","External Factors","","","","","Action Required","2020-12-30T23:59:35","","Completed","2020-12-05T23:59:35","No","No","No","Internal"]
[null,null,null,15575,null,"107_Tue Dec 08 2020 10:43:34 GMT+0000","2020-11-28T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","FWG production  too low- Evaporator and condenser to be cleaned","E/R - Aux. Mach.","Eng. / Strg. Comp.","External Factors,Equipment Related","","","","","Chemical cleaned the evaporator / condenser @ 20201222 Richards Bay anchor. Working @ 20201227, but found product little less than when ship ballast condition.","2020-12-30T23:59:35","","Completed","2020-12-21T23:59:35","No","No","No","Internal"]
[null,null,null,15455,null,"107_7/12/2020 9:10:02 PM","2020-12-02T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Steam pipe connected to EGE soot blowier damaged & broken","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Dec-08th - Pipe renewed.","2021-01-04T23:59:35","","Completed","2020-12-07T23:59:35","No","No","No","Internal"]
[null,null,null,14674,null,"107_Mon Nov 16 2020 11:12:57 GMT+0000","2020-12-06T23:59:35","Defect,Observation","Ship Staff","Ship Staff Insp.","Three (3) mooring winches brake linings are not good, required renewal","Deck - Mooring Machinery","Mooring","Equipment Related","","","","","plan renewal by this month","2020-12-29T23:59:35","","Completed","2020-11-11T23:59:35","No","No","No","Internal"]
[null,null,null,16300,null,"107_31/12/2020 4:13:02 AM","2020-12-11T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Digital books ENP just have software, due to ship signal poor, not can be download digital books and IMO digital books no have books license and need books list)","Navigation - Others","Navigation","Equipment Related","","","","","COMPLETED DOWNLOAD","2021-01-30T23:59:35","","Completed","2020-12-31T23:59:35","No","No","No","Internal"]
[null,null,null,16302,null,"107_31/12/2020 4:18:21 AM","2020-12-11T23:59:35","Observation","Ship Staff","Ship Staff Insp.","BNWAS: Bracket of control devices which is located on starboard side of the bridge, bracket is corroded and damage New holding plate to be fitted, apply paint then fit box properly.","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","External Factors","","","","","Will fabricated newly bracket etc.","2021-01-30T23:59:35","","Completed","2021-02-28T23:59:35","No","No","No","Internal"]
[null,null,null,15581,null,"107_12/13/2020 5:06:01 AM","2020-12-11T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Digital books ENP just have software, due to ship signal poor, not able to download digital books and IMO digital books does not have books license and need books list","Navigation - Others","Navigation","Inappropriate Procedure","","","","","we need shore download books send to ship NAVBOX","2020-12-24T23:59:35","","Completed","2020-12-15T23:59:35","No","No","No","Internal"]
[null,null,null,15582,null,"107_12/13/2020 11:31:33 AM","2020-12-11T23:59:35","Observation","Ship Staff","Ship Staff Insp.","BNWAS: Bracket  of control devices which is located on starboard side of the bridge, bracket is corroded and damage New holding plate to be fitted, apply paint then fit box properly.","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","External Factors","","","","","New holding plate to be fitted, apply paint then fit box properly.","2020-12-24T23:59:35","","Completed","2020-12-16T23:59:35","No","No","No","Internal"]
[null,null,null,14684,null,"107_Mon Nov 16 2020 11:28:17 GMT+0000","2021-01-10T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Port Windlass unable to heave up Anchor cable at 4 shackles on Deck. Recorded Date changed as spares not rec'd . Actual date 27th Sept'21","Deck - Mooring Machinery","Mooring","Equipment Related","","","","","Hyd Motor renewed. Working Better. one New Block found in Midship Store. Same replaced and noticed working well. Non similar one landed in ingapore for replacement.","2022-01-30T23:59:35","ANTW210144","Completed","2022-11-30T23:59:35","No","No","No","Internal","Pls update spare receiving status and get the job done ASAP"]
[null,null,null,23962,null,"107_2/16/2022 3:43:49 PM","2021-01-11T23:59:35","Defect","Ship Staff","Ship Staff Insp.","SLUDEG PUMP SAFETY VALVE INOPERATIONAL","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","","","","","Overhauled","2022-03-29T23:59:35","","Completed","2021-05-11T23:59:35","No","No","No","Internal"]
[null,null,null,18325,null,"107_2/2/2021 11:00:20 PM","2021-01-31T23:59:35","Observation","Ship Staff","Ship Staff Insp.","No6 hatch cover can't opened by fixing hyd.pump.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","Raised spare requisition ANTW215029. Try to adjust the safety valve of pump. Can operate No6 hatch cover. Renewed the pump when receipt.","2021-03-30T23:59:35","Waiting spare requisition ANTW215029.","Completed","2021-03-19T23:59:35","No","No","No","Internal"]
[null,null,null,15562,null,"107_Tue Dec 08 2020 07:50:58 GMT+0000","2021-03-01T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","A/E F.O. viscosity meter assy removed by UNIMARINE and off landed at Singapore for repair.","E/R - Pumps","Eng. / Strg. Comp.","External Factors,Equipment Related","","","","","AT Singapore shore engineer come on board.Checked and test Running is normal at that time.l","2021-05-07T23:59:35","","Completed","2021-05-07T23:59:35","Yes","No","No","Internal","Visco meter overhauled and supplied to vsl.  Still it is malfunctioning. It will be dealt with during docking in June'21"]
[null,null,null,15237,null,"107_Wed Nov 25 2020 05:57:32 GMT+0000","2021-03-03T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Topping up air compressor required to be overhauled due to poor performance","E/R - Air Comp.","Eng. / Strg. Comp.","External Factors","","","","","Complet overhauling done by ship staff and put in use. ","2021-06-03T23:59:35","ANTW 205077","Completed","2021-09-19T23:59:35","No","No","No","Internal","spare supplied, please update"]
[null,null,null,15557,null,"107_Tue Dec 08 2020 07:38:04 GMT+0000","2021-03-04T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Funnel deck  light holder  3 nos supports corroded and wasted, same to be renewed.","Deck - Pipe / Fittings","General Appearance","External Factors","","","","","The spare  re-supplied on S.G.P . The light renewed completed.The light holder 3 nos supports re-rust and paint.","2021-06-04T23:59:35","","Completed","2021-05-16T23:59:35","Yes","No","No","Internal","Requisition will be supplied at next convenient port."]
[null,null,null,15242,null,"107_Wed Nov 25 2020 06:08:16 GMT+0000","2021-03-09T23:59:35","Observation","Ship Staff","Ship Staff Insp.","A/E No.3 fuel injectors to be renewed as it is overdue.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","All renewed during Decarb of the DG3 in DD.","2021-06-08T23:59:35","ANTW205073, 215034","Completed","2021-09-08T23:59:35","No","No","No","Internal","Please prepare one sets of fuel injector and replace  all six  units fuel injectors."]
[null,null,null,15580,null,"107_12/13/2020 4:53:59 AM","2021-03-17T23:59:35","Defect","Ship Staff","Ship Staff Insp.","VDR sometimes will display rudder error?timeout on SI17 rudder indicator","Navigation - VDR / BNWAS","Navigation","Equipment Related","","","","","Rectified in Dry Dock","2021-06-14T23:59:35","","Completed","2021-09-08T23:59:35","No","No","No","Internal","please keep monitor and will solve it during dry dock"]
[null,null,null,16301,null,"107_31/12/2020 4:22:32 AM","2021-03-21T23:59:35","Observation","Ship Staff","Ship Staff Insp.","No2 FO supply pump for HFO purifier: mech.seal leaking.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","","","","","Waiting spares antw215016. Anyway, exchanged by old mech.seal & no leaking now.","2021-06-16T23:59:35","ANTW 027-2020 send to office @ 20201228.","Completed","2021-03-08T23:59:35","No","No","No","Internal","Spares will be supplied at next convenient port. owner will supply"]
[null,null,null,15567,null,"107_Tue Dec 08 2020 08:26:47 GMT+0000","2021-04-04T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Provision Crane (S): Found hoist and slewing limit not working, not able to carry out further trouble shooting due to no platform for the winch limit. Jib slewing limit is badly corroded and jammed, needs to be replace with new. Limit switch cam corroded and need change. Manual control lever not able to return to center upon release, and externally badly corroded. All hoses need to be renewal.  Cylinder Load holding valve requires to be renewed. Internal slewing bearing gear dry and need greasing. Winch standing platform is badly corroded. Spares will be sourced to rectify above mentioned faults.","Deck - Machinery","General Appearance","Equipment Related","","","","","The renewed hoses when D-docking.\n\n\n\n\n\n\n\nRectified in DD.","2021-06-09T23:59:35","ANTW 205083","Completed","2021-09-08T23:59:35","Yes","No","No","Internal","Pls do check and advise  Job will be carried out during docking"]
[null,null,null,19636,null,"107_6/10/2021 10:35:55 PM","2021-05-30T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Engineering Audit","Dump condenser/drain cooler in poor condition,both sidecovers temporary re-conditioned,7 pcs of tube blocked","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","New Dump Condenser Installed","2021-08-09T23:59:35","","Completed","2021-08-25T23:59:35","Yes","No","No","Internal","will carry out in DD."]
[null,null,null,19733,null,"107_6/17/2021 8:37:00 PM","2021-06-14T23:59:35","Defect,Observation","Class Surveyor","Others (Eg. Insurance etc.)","No.1 cargo hatch cover operating station leakage excessive due to poor condition of valve plate","Deck - Pipe / Fittings","General Appearance","Equipment Related","","","","","Job attended in DD","2021-07-14T23:59:35","","Completed","2021-03-08T23:59:35","No","No","No","External","will supply spare parts in convenient port to replace damage one"]
[null,null,null,20168,null,"107_7/14/2021 3:52:31 AM","2021-07-13T23:59:35","Observation","Ship Staff","Ship Staff Insp.","ECR air condition plant in poor condition both compressor and condenser,gas leakage in several places","Elect. Mach. & Equip.,Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","raise spare parts,replace the compressor and condenser when dry docking","2021-08-14T23:59:35","ANTW210075","Completed","2021-03-08T23:59:35","No","No","No","Internal","will carry out in DD"]
[null,null,null,15565,null,"107_Tue Dec 08 2020 08:21:34 GMT+0000","2021-07-26T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Stbd Windlass: Main shaft bearing is badly worn out which causing excessive shaft movement.","Deck - Mooring Machinery","Mooring","Equipment Related","","","","","Inspected in DD and found in stasfactory condition.","2021-09-29T23:59:35","","Completed","2021-09-04T23:59:35","Yes","No","No","Internal","Pls submit R.O. for the spare parts. Job to be carried out during docking."]
[null,null,null,19527,null,"107_12-05-2021 08:28:32","2021-08-09T23:59:35","Defect","Ship Staff","Engineering Audit","G/E fuel oil visocity controller steam adjust valve cann't move.Adjust set valve but The Control air cann't move .","Deck - Pipe / Fittings,E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Job attended in Dry Dock by IMA, controllers under observations","2021-10-30T23:59:35","","Completed","2021-09-07T23:59:35","No","No","No","Internal","please update status after service attending in Singapore"]
[null,null,null,20169,null,"107_7/14/2021 8:31:57 PM","2021-08-09T23:59:35","Observation","Ship Staff","Ship Staff Insp.","NO.2-5 hatch coaming scattered spot rust should be hydro blasted and painted","Deck - Pipe / Fittings","General Appearance","External Factors","","","","","Derusting and painting carried out.Job completed.","2022-03-29T23:59:35","","Completed","2022-03-26T23:59:35","No","No","No","Internal","please carry out as plan and keep update"]
[null,null,null,20603,null,"107_8/15/2021 07:37:51","2021-08-14T23:59:35","Observation","Ship Staff","Ship Staff Insp.","S/S UPPER NAV.LIGHT IS DAMAGE","Navigation - Others","Navigation","External Factors","","","","","RAISED RO ANTW210104","2021-08-30T23:59:35","","Completed","2021-09-04T23:59:35","No","No","No","Internal","please get it done in ship yard"]
[null,null,null,20604,null,"107_8/15/2021 12:34:11","2021-08-14T23:59:35","Defect","Ship Staff","Ship Staff Insp.","ELECTRICAL HORN PANEL OUT OF ORDER","Navigation - Others","Navigation","Inappropriate Procedure","","","","","RAISED RO ANTW210045","2021-08-30T23:59:35","ANTW210045","Completed","2021-08-22T23:59:35","No","No","No","Internal","will supplied spare in yard. otherwise please make sure to rectify prior to leave from yard"]
[null,null,null,20605,null,"107_8/15/2021 12:49:27","2021-08-14T23:59:35","Observation,Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","S-BAND / X-BAND RADAR POOR DETECTION FAIL ","Navigation - RADAR","Navigation","Equipment Related","","","","","INFORMED TECH.SUPT. PRAVEEN GANDHI AND FOR SERVICE IN DD DATED 15 AUG.2021","2021-08-30T23:59:35","","Completed","2021-08-30T23:59:35","Yes","No","No","Internal","please get the job done in shipyard"]
[null,null,null,20607,null,"107_8/15/2021 13:05:27","2021-08-14T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ECDIS NO.2  TO CHECK NAVTEX SENSOR & FUN FOR MONITOR FOR COOLING SHOWING ERROR","Navigation - ECDIS","Navigation","Equipment Related","","","","","INFORMED TECH.SUPT. PRAVEEN GANDHI & BY OBSERVATION INTERNAL AUDIT OF CAPT. KHOSA DATED 8 AUG.2021","2021-08-30T23:59:35","","Completed","2021-09-06T23:59:35","Yes","No","No","Internal","please get the job done in shipyard"]
[null,null,null,15568,null,"107_Tue Dec 08 2020 08:30:11 GMT+0000","2021-08-14T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Ship Staff Insp.","AE LO purifier temperature controller require spare for repairs, same being sourced. Two nos of automatic steam control valve overhauled for HFO purifier as same found erratic.","E/R - Purifier,Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","Job attended by IMA, controller under observations","2021-10-30T23:59:35","","Completed","2021-09-07T23:59:35","Yes","No","No","Internal","please update status"]
[null,null,null,15569,null,"107_Tue Dec 08 2020 10:33:21 GMT+0000","2021-08-14T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Ship Staff Insp.","Main deck, cross decks, poop decks and forecastle deck sighted scattered spot rust, same to be hydro blasted and painted.","Deck - Pipe / Fittings","General Appearance","External Factors","","","","","Deck side hyrdoblasted and painting carried out.Job completed.","2022-03-29T23:59:35","","Completed","2022-03-21T23:59:35","No","No","No","Internal","Vsl to keep office updated with weekly reporting for maintenance progress."]
[null,null,null,15574,null,"107_Tue Dec 08 2020 10:41:28 GMT+0000","2021-08-26T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Ship Staff Insp.","Crew laundry room upper deck common toilets floor tiles rust stained and same required to be renewed.","Accommodation","General Appearance","External Factors","","","","","Material rec'd, work is in progress","2021-12-29T23:59:35","","Completed","2022-01-01T23:59:35","Yes","No","No","Internal","please get the job done ASAP"]
[null,null,null,22784,null,"107_17-Nov-21 19:21:50","2021-08-28T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","TO BE CLEAN EXHAUST VENTILATION IN GALLEY. TO RENEW VARIOUS RUBBER PACKING ON CREW’S MAIN DOOR.","Accommodation","MLC Related","Human Error","","","","","Exhaut ventilation cleaned and rubber packing renewed","2021-11-28T23:59:35","","Completed","2021-10-05T23:59:35","No","No","No","Internal"]
[null,null,null,22785,null,"107_17-Nov-21 19:24:02","2021-08-28T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","FUNNEL PAINTING TO BE COMPLETED.","Miscellaneous","General Appearance","Human Error","","","","","Funnel painted","2021-11-28T23:59:35","","Completed","2021-10-13T23:59:35","No","No","No","Internal"]
[null,null,null,22786,null,"107_17-Nov-21 19:57:28","2021-08-28T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Topping up compressor not working","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Overhauled and now in good working condition","2021-11-28T23:59:35","","Completed","2021-10-04T23:59:35","No","No","No","Internal"]
[null,null,null,22787,null,"107_17-Nov-21 19:59:56","2021-08-28T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","AE 2 ACB OCR to replace with spare ocr received in yard","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","OCR replaced","2021-11-28T23:59:35","","Completed","2021-10-04T23:59:35","No","No","No","Internal"]
[null,null,null,22788,null,"107_17-Nov-21 20:03:54","2021-08-28T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","FO sludge tank HL alarm inoperational","Critical Equip.,Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","Alarm reactified","2021-10-29T23:59:35","","Completed","2021-10-01T23:59:35","No","No","No","Internal"]
[null,null,null,22789,null,"107_17-Nov-21 20:24:37","2021-08-28T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Main Air compressor to overhaul, as takes long time to press up","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related","","","","","Overhauled and working in good condition","2021-11-28T23:59:35","","Completed","2021-10-09T23:59:35","No","No","No","Internal"]
[null,null,null,22790,null,"107_17-Nov-21 20:26:39","2021-08-28T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Sea chest MGPS anodes to replace by vessel staff","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Anodes replaced","2021-11-28T23:59:35","","Completed","2021-10-12T23:59:35","No","No","No","Internal"]
[null,null,null,22791,null,"107_17-Nov-21 20:29:22","2021-08-28T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Main Air compressor intermittently trips on High air temp, required overhauling of compressor, major spares located, consumables to check ","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related","","","","","Overhauled and working in good order","2021-11-28T23:59:35","","Completed","2021-10-04T23:59:35","No","No","No","Internal"]
[null,null,null,22792,null,"107_17-Nov-21 20:31:43","2021-08-28T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ME maouvering area to be clean and neat","Miscellaneous","General Appearance","Human Error","","","","","Cleaned and painted","2021-11-28T23:59:35","","Completed","2021-10-03T23:59:35","No","No","No","Internal"]
[null,null,null,22779,null,"107_17-Nov-21 18:55:39","2021-08-28T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","DANGER ZONE MARKING WITH TIGER STRIPE.","Miscellaneous","Navigation","Human Error","","","","","Danger zones marked with tiger strips","2021-11-28T23:59:35","","Completed","2021-10-13T23:59:35","No","No","No","Internal"]
[null,null,null,22780,null,"107_17-Nov-21 19:05:51","2021-08-28T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","EMERGENCY GENERATOR VENTILATION PACKING RUBBER TO BE REPLACED.","Miscellaneous","General Appearance","Human Error","","","","","Rubber packing changed","2021-11-28T23:59:35","","Completed","2021-10-09T23:59:35","No","No","No","Internal"]
[null,null,null,22781,null,"107_17-Nov-21 19:11:51","2021-08-28T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","FUNNEL EXHAUST PIPES TO BE DE-RUSTED(SCRIPPED ONLY) AND PAINTED.","Miscellaneous","General Appearance","Human Error","","","","","Funnel exhaust pipes scrapped and painted","2021-11-28T23:59:35","","Completed","2021-10-12T23:59:35","No","No","No","Internal"]
[null,null,null,22782,null,"107_17-Nov-21 19:16:09","2021-08-28T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","PROVISION CRANES P/S WASTED FLATFORMS TO BE RENEW, DE-RUSTED/PAINTED.","Deck - Machinery","General Appearance","Human Error","","","","","Platforms renewed","2021-11-28T23:59:35","","Completed","2021-10-02T23:59:35","No","No","No","Internal"]
[null,null,null,22783,null,"107_17-Nov-21 19:18:56","2021-08-28T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","TO RECONDITIONED ALL CONTROL STANDS OF HYDRAULIC HATCH COVERS, TO BE DE-RUSTED/PAINTED.","Deck - Pipe / Fittings","General Appearance","Human Error","","","","","Control stands reconditioned","2021-11-28T23:59:35","","Completed","2021-10-19T23:59:35","No","No","No","Internal"]
[null,null,null,15559,null,"107_Tue Dec 08 2020 07:45:26 GMT+0000","2021-08-30T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Ship Staff Insp.","Deck air lines sighted corroded in various places, all corroded pipes to be renewed.","Deck - Pipe / Fittings","General Appearance","External Factors","","","","","80% job completed.work in progress.","2022-03-29T23:59:35","ANTW210015.","Completed","2022-03-26T23:59:35","Yes","No","No","Internal","please update status"]
[null,null,null,21889,null,"107_15/10/2021 23:01:42","2021-09-08T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Boiler Feed Water Pump #1 and #2 Seals are not in place.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Both Pumps overhauled with Mechanical seal ","2021-11-14T23:59:35","ANTW215131","Completed","2021-11-14T23:59:35","No","No","No","Internal","please update status"]
[null,null,null,21890,null,"107_15/10/2021 23:27:29","2021-10-09T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Port Side Bunker Davit Pnuematic Motor non operational","Deck - Machinery","Eng. / Strg. Comp.","Equipment Related","","","","","Overhauled and made operational","2021-11-19T23:59:35","","Completed","2021-02-10T23:59:35","No","No","No","Internal","please keep update status"]
[null,null,null,21892,null,"107_15/10/2021 23:19:47","2021-10-12T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","#2 Main Cooling SW Pump Motor Burnt","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","Motor renewed with a new spare rec'd","2021-10-10T23:59:35","ANTW210165","Completed","2021-05-10T23:59:35","No","No","No","Internal","noted, will supply in convenient port"]
[null,null,null,14667,null,"107_Mon Nov 16 2020 10:58:32 GMT+0000","2021-10-31T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Main engine RHRS counter and REV counter are Not working. Total ME RHRS on 9th Sept'21 is 98251 which recorded manually. Recorded Date changed as spares not rec'd . Actual date 9th Sept'21","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","Rhrs entered manually.Will rectify when new spare recieved.","2022-03-30T23:59:35","ANTW215012","Completed","2022-03-26T23:59:35","No","No","No","Internal","will supply in convenient port, please update spare receiving status"]
[null,null,null,14671,null,"107_Mon Nov 16 2020 11:06:02 GMT+0000","2021-10-31T23:59:35","Defect","Ship Staff","Ship Staff Insp.","No.1 HFO purifier temp control valve malfunctioning. No.2 HFO Purifier Temp. controller complete device found missing. Recorded Date changed as spares not rec'd . Actual date 9th Sept'21","E/R - Purifier","Eng. / Strg. Comp.","Equipment Related","","","","","Temp Controller replaced with new.Now working satisfactory.","2022-03-30T23:59:35","ANTW210188","Completed","2022-03-21T23:59:35","No","No","No","Internal","Please  do check and  advise  in details what is the problem. on the temp control valve."]
[null,null,null,21887,null,"107_15/10/2021 23:40:25","2021-10-31T23:59:35","Defect","Ship Staff","Ship Staff Insp.","ME and DG Viscosity controller.malfunction. Recorded Date changed as spares not rec'd . Actual date 22 Sept' Sept'21","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","New controler recieved.Found problem with control valve.Controller working fine.Control valve to be checked.\n\n\n\n","2022-03-30T23:59:35","ANTW210178","Completed","2022-03-26T23:59:35","No","No","No","Internal","will process and supply in convenient port"]
[null,null,null,21888,null,"107_15/10/2021 23:09:56","2021-10-31T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Boiler FO Flow meter completely damaged. ME and DG FO flowmeter not showing correct quantity.Recorded Date changed as spares not rec'd . Actual date 22nd Sept'21","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Checking all Bunker tank quantity manually at every noon and showing appropriate consumption based on the ME speed and DG load and Boiler RHRS. Requisition will be done as per office instruction.","2022-03-30T23:59:35","ANTW210179","Completed","2022-07-02T23:59:35","No","No","No","Internal","will process and supply in convenient port"]
[null,null,null,21891,null,"107_15/10/2021 23:16:05","2021-10-31T23:59:35","Non Conformity","Ship Staff","Ship Staff Insp.","Commutator in Galley found missing. Recorded Date changed as spares not rec'd . Actual date 29th Sept'21","Accommodation","MARPOL Related","Equipment Related","","","","","At present food being disposed in accordance with MARPOL Reg.Will isnatll spare once received.","2022-03-30T23:59:35","ANTW210166","Completed","2022-03-30T23:59:35","No","No","No","Internal","will process and supply in convenient port"]
[null,null,null,19637,null,"107_11/6/2021 8:19:59 AM","2021-11-05T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Part of WBT manholes?14pcs? and HFO manholes?2pcs? serious corrosion become weak .It mus be renewwed","Deck - Pipe / Fittings","General Appearance","External Factors","","","","","Bunker Tanks manholes renewed and WBT manhole gaskets renewed in DD","2021-11-05T23:59:35","","Completed","2021-08-29T23:59:35","Yes","No","No","Internal","please de-rust and paint first. will carry out renew in DD, please including it in the DD spec"]
[null,null,null,22774,null,"107_11/30/2021 10:49:21 PM","2021-11-10T23:59:35","Defect","Ship Staff","Ship Staff Insp.","ME JACKET COOLING WATER TEMPERATURE CONTROLER NOT WORKING","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","Controler replaced with new spare.Now working satisfactory.","2022-03-30T23:59:35","ANTW210189","Completed","2022-03-22T23:59:35","No","No","No","Internal","will process and supply in convenient port"]
[null,null,null,22775,null,"107_11/30/2021 10:42:28 PM","2021-11-10T23:59:35","Defect","Ship Staff","Ship Staff Insp.","OVER CURRENT RELAY FOR DG #3 ACB MALFUNCTION","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","Renewed with a spare one.","2022-02-27T23:59:35","ANTW210187","Completed","2022-09-01T23:59:35","No","No","No","Internal","will process and supply in convenient port"]
[null,null,null,22776,null,"107_11/30/2021 10:53:59 PM","2021-11-13T23:59:35","Defect","Ship Staff","Ship Staff Insp.","ME FO SERV. TANK TEMP. CONTROLLER FOR STEAM VALVE NOT WORKING","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Temp being well maintained with manual control valve.","2022-03-30T23:59:35","ANTW210190","Completed","2022-03-26T23:59:35","No","No","No","Internal","will process and supply in convenient port"]
[null,null,null,20606,null,"107_8/15/2021 12:55:44","2021-11-14T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","BRIDGE WINDOW WIPER 2 OF 3 OUT OF ORDER","Navigation - Others","Navigation","Equipment Related","","","","","Spares on order.Job will be done once spares are received.","2022-03-30T23:59:35","ANTW210119","Completed","2022-03-30T23:59:35","Yes","No","No","Internal","spare will supply in convenient port"]
[null,null,null,22777,null,"107_11/30/2021 11:26:54 PM","2021-11-18T23:59:35","Defect","Ship Staff","Ship Staff Insp.","HFO SETT. & SERV. TANK LEVEL GAUGE NOT WORKING","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Sounding are taken manually.Will install gauages when supplied.","2022-03-30T23:59:35","ANTW210201","Completed","2022-03-29T23:59:35","No","No","No","Internal","will process and supply in convenient port"]
[null,null,null,22778,null,"107_11/30/2021 11:30:50 PM","2021-11-20T23:59:35","Defect","Ship Staff","Ship Staff Insp.","EMERGENCY GENERATOR HYDRAULIC STARTER SYSTEM MALFUNCTION","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","Replaced starter with new spare.Now working satisfactory.","2022-03-30T23:59:35","ANTW210198","Completed","2022-03-15T23:59:35","No","No","No","Internal","will process and supply in convenient port"]
[null,null,null,27004,null,"107_Mon Sep 26 2022 03:34:42 GMT+0000","2021-11-24T23:59:35","Observation","PSC Insp.","PSC Inspection","Annual test of loading computer is not presented during inspection time","Cargo Mach.","Cargo / Ballast Systems","","","","Cargo operations including equipment","","","2021-12-19T23:59:35","","Completed","2021-12-19T23:59:35","No","No","No","External"]
[null,null,null,27005,null,"107_Mon Sep 26 2022 03:35:53 GMT+0000","2021-11-24T23:59:35","Observation","PSC Insp.","PSC Inspection","Requirement to provide safe carriage of cargo are underachieved ( four sets of protective clothing and two SCBA","Cargo Mach.","Cargo / Ballast Systems","","","","Cargo operations including equipment","","","2021-12-19T23:59:35","","Completed","2021-12-16T23:59:35","No","No","No","External"]
[null,null,null,27006,null,"107_Mon Sep 26 2022 03:37:17 GMT+0000","2021-11-24T23:59:35","Observation","PSC Insp.","PSC Inspection","Overfill boxes are not marked as required","","","","","","Pollution Prevention","","","2021-12-19T23:59:35","","Completed","2021-12-16T23:59:35","No","No","No","External"]
[null,null,null,27007,null,"107_Mon Sep 26 2022 03:38:49 GMT+0000","2021-11-24T23:59:35","Observation","PSC Insp.","PSC Inspection","Reflective tapes on life boat bottom are missing","LSA / FFA","Safety / LSA / FFA","","","","Life saving appliances","","","2021-12-19T23:59:35","","Completed","2021-12-16T23:59:35","No","No","No","External"]
[null,null,null,23825,null,"107_2/1/2022 5:09:54 PM","2021-11-30T23:59:35","Observation","Ship Staff","Ship Staff Insp.","ME Liner Measuring tool Missing","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Liner calibration tool on order.","2022-03-30T23:59:35","ANTW220030","Completed","2022-03-13T23:59:35","No","No","No","Internal","will process RO and supply in convenient port"]
[null,null,null,23826,null,"107_2/1/2022 5:17:52 PM","2021-11-30T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Wiper Cabin Vaccum Toilet system inoperational","Accommodation","MLC Related","Equipment Related","","","","","Control system and water suppy unit checked. Found Ok. Sewage outlet branch pipe is chocked. Planning to renew after Singapore","2022-02-27T23:59:35","","Completed","2022-12-02T23:59:35","No","No","No","Internal","please carry out ASAP and update next time"]
[null,null,null,23827,null,"107_2/1/2022 5:34:01 PM","2021-11-30T23:59:35","Defect","Ship Staff","Ship Staff Insp.","#2 DG , #4 unit Fuel Pump connecting pipe Arm seat surface worn down / leaking","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Used spare found in store.It was in good condition.Same replaced.Now no leak.","2022-03-30T23:59:35","ANTW220004","Completed","2022-03-18T23:59:35","No","No","No","Internal","will supply spare in next convenient port"]
[null,null,null,23119,null,"107_14/12/2021 14:57:23","2021-12-08T23:59:35","Defect","Ship Staff","Ship Staff Insp.","FO Bunker Tank STBD filling valve is too tight to operate","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","Equipment Related","","","","","Bunker valve eased up in place.Now freely moving.","2022-03-30T23:59:35","ANTW220012","Completed","2022-03-18T23:59:35","No","No","No","Internal","please carry out maintenance for the valve. it is not only require to renew the valve to solve the issue. RO will process and supply in convenient port."]
[null,null,null,23120,null,"107_14/12/2021 15:43:12","2021-12-09T23:59:35","Critical Equipment","Ship Staff","Ship Staff Insp.","Auto STBY Pump starting not happening for ME LO Pump, Cam Shaft LO Pump and MCSW Pump.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","All pumps Auto change over Module replaced with new spares.Now working satisfactory.","2022-03-30T23:59:35","ANTW220001","Completed","2022-03-30T23:59:35","No","No","No","Internal","please check and confirm. raise RO if required"]
[null,null,null,23121,null,"107_14/12/2021 14:53:23","2021-12-10T23:59:35","Defect","Ship Staff","Ship Staff Insp.","While carrying out yearly pressure test of HFO bunker line, found section of pipe holed at 3 Bar air pressure","Deck - Pipe / Fittings","MARPOL Related","Equipment Related","","","","","Fabrication of 2 section of line completed. Other weaker section to identify and renew","2021-12-16T23:59:35","","Completed","2021-12-16T23:59:35","No","No","No","Internal","please update status for the job."]
[null,null,null,23122,null,"107_12/15/2021 7:39:49 PM","2021-12-11T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Port Steering Gear Pump Oil Seal leaking. (Pls. note this issue is there since Dry Dock Sept'21)","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Leak is very minimal.Once spare seal received we will change it.","2022-03-30T23:59:35","ANTW210200","Completed","2022-03-25T23:59:35","No","No","No","Internal","will supply spare in convenient port"]
[null,null,null,23123,null,"107_14/12/2021 15:04:20","2021-12-11T23:59:35","Non Conformity","Ship Staff","Ship Staff Insp.","Port FW tank Sight Glass Bottom Valve is ship's made one which is always in open position","Hull & Tanks","Safety / LSA / FFA","Equipment Related","","","","","Emptied out the tank and overhauled  the valve. ","2022-01-30T23:59:35","","Completed","2021-12-28T23:59:35","No","No","No","Internal","please check if spare not available raise RO"]
[null,null,null,23124,null,"107_14/12/2021 15:48:07","2021-12-11T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Both Provision Cranes Safety limit switches are not working","Deck - Machinery","Safety / LSA / FFA","Equipment Related","","","","","Port side crane switch renewed and STBD side Switcheased up","2022-01-30T23:59:35","","Completed","2022-01-05T23:59:35","No","No","No","Internal","please carry out ASAP and update"]
[null,null,null,23125,null,"107_14/12/2021 15:18:54","2021-12-12T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Sewage Holding Tank level Gauge is not working","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Tank level gauge removed and cleaned.now working satisfactory.","2022-03-30T23:59:35","ANTW220003","Completed","2022-03-12T23:59:35","No","No","No","Internal","spare will supply in convenient port"]
[null,null,null,23126,null,"107_14/12/2021 15:27:34","2021-12-12T23:59:35","Defect","Ship Staff","Ship Staff Insp.","#8 Hatch cover operation is very slow.","Deck - Machinery","Cargo / Ballast Systems","Equipment Related","","","","","Found no issues with Flow control valve. Tried out with Emergency pump found working normal. Old block will be landed for repair as per Master's decision.","2021-12-17T23:59:35","ANTW215150","Completed","2021-12-28T23:59:35","No","No","No","Internal","please update status."]
[null,null,null,23127,null,"107_14/12/2021 16:37:07","2021-12-13T23:59:35","Defect","Ship Staff","Ship Staff Insp.","ER Toilet Vaccum system operating mechanism altered and fabricated with ordinary valve. Vaccum getting released and alarm on the panel","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Replaced the control system, water controller and repair the Push button switch. Working normal. ","2021-12-30T23:59:35","ANTW210228","Completed","2021-12-19T23:59:35","No","No","No","Internal","will supply spares in convenient port"]
[null,null,null,23128,null,"107_14/12/2021 16:42:57","2021-12-13T23:59:35","Defect","Ship Staff","Ship Staff Insp.","EGE soot Blower not functioning / Rotating","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","Removed and overhaul done during Suez anchorage.","2021-12-30T23:59:35","","Completed","2021-12-14T23:59:35","No","No","No","Internal","please carry out and update"]
[null,null,null,23129,null,"107_14/12/2021 16:54:31","2021-12-13T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Boiler Mountings such as air vent valve, gauge valve found not installed.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","Instaledl the required valves at Port Said in Suez after depressurising the boiler.","2021-12-19T23:59:35","","Completed","2021-12-18T23:59:35","No","No","No","Internal","please carry out and update. item will due soon"]
[null,null,null,23130,null,"107_14/12/2021 17:01:36","2021-12-13T23:59:35","Observation","Ship Staff","Ship Staff Insp.","AE1 RPM Indicator at the Engine side shows lesser (700) than rated RPM (900)","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","New spare found in box.Same replaced.Now working satisfactory.","2022-03-30T23:59:35","ANTW220004","Completed","2022-03-22T23:59:35","No","No","No","Internal","will process and supply in convenient port"]
[null,null,null,23348,null,"107_1/1/2022 5:14:21 PM","2021-12-31T23:59:35","Defect","Ship Staff","Ship Staff Insp.","DG D.O. Pump mechanical seal leaking","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","DO leak is very minimal as pump runs only during start and stop of AE.Will change seal after receiving spare.","2022-03-30T23:59:35","ANTW220004","Completed","2022-03-30T23:59:35","No","No","No","Internal","will process and supply in convenient port"]
[null,null,null,23349,null,"107_1/1/2022 7:42:18 PM","2021-12-31T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Gang way Motor (S) not holding in its position","Deck - Machinery","General Appearance","Equipment Related","","","","","Gangway motor overhauled.Now working satisfactory.","2022-03-30T23:59:35","ANTW220010","Completed","2022-06-02T23:59:35","No","No","No","Internal","will process and supply in convenient port"]
[null,null,null,23350,null,"107_1/1/2022 7:46:48 PM","2021-12-31T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Hydro Blaster triggering pressure fluctuate","Deck - Machinery","Cargo / Ballast Systems","Equipment Related","","","","","Trigger overhauled.now getting correct pressure.","2022-03-30T23:59:35","ANTW220009","Completed","2022-03-12T23:59:35","No","No","No","Internal","will process and supply in convenient port"]
[null,null,null,23478,null,"107_1/14/2022 4:07:30 PM","2021-12-31T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Boiler FO low Pr. Change over Pr. Switch faulty","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","Spare Req has been made.Low pressure change over switch isolated.","2022-03-30T23:59:35","ANTW220029","Completed","2022-03-30T23:59:35","No","No","No","Internal","will process and supply in convenient port"]
[null,null,null,23479,null,"107_1/14/2022 4:15:01 PM","2021-12-31T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Foam Nozzle leak due to damaged valves in SG room","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","Fire pump run for one hour.No leak was observed at any Foam nozzle in engine room.","2022-02-27T23:59:35","ANTW220057","Completed","2022-03-30T23:59:35","No","No","No","Internal","job still pending? if completed please fill up complete date and close the defect. refer previous comments. please overhaul the valve and lap to rectify the leakage. spare will supply next convenient port."]
[null,null,null,23482,null,"107_1/14/2022 4:24:18 PM","2021-12-31T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Galley AC Non operational due to Cooling water line issue.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","New line fabricated for condensor. Cond. cleaned. System checked, Gas charged, safet tested, started and put in use. Leak test done. All OK","2022-03-30T23:59:35","","Completed","2022-02-20T23:59:35","No","No","No","Internal","please carry out before due date"]
[null,null,null,23483,null,"107_1/14/2022 4:40:30 PM","2021-12-31T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Sludge Pump Relief valve malfunction","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Inside parts damaged. Raised a requisition.","2022-03-30T23:59:35","ANTW220021","Completed","2022-06-02T23:59:35","No","No","No","Internal","please carry out within the target date"]
[null,null,null,23485,null,"107_1/14/2022 4:20:14 PM","2021-12-31T23:59:35","Defect","Ship Staff","Ship Staff Insp.","STBD Windlass Flushing valve jammed","Deck - Mooring Machinery","Mooring","Equipment Related","","","","","Easing up is in progress","2022-02-27T23:59:35","","Completed","2022-12-02T23:59:35","No","No","No","Internal","please carry out overhaul and update"]
[null,null,null,23954,null,"107_2/16/2022 12:25:07 PM","2022-01-01T23:59:35","Guarantee Claim","Ship Staff","Ship Staff Insp.","Gym Equipment parts missing, delivered in DD.","Miscellaneous","MLC Related","Equipment Related","","","","","Message sent to 26th Dec'21. Weight System Exerciser, Maker WEIDERPRO 6900, Model no. 831.14922.2, supplied in Dubai DD, in Sept’21 does not contain all the parts","2022-05-30T23:59:35","Procure Dept. knows the RO number","Completed","2022-03-12T23:59:35","No","No","No","Internal","please remind procure to finalized the issue. don't keep this as DDRL in pending."]
[null,null,null,23695,null,"107_17-Jan-22 21:44:01","2022-01-05T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Deck pipe mechanical vent mushroom head damper wheel seized","Deck - Pipe / Fittings","General Appearance","Human Error","","","","","Repaired","2022-03-08T23:59:35","","Completed","2022-01-14T23:59:35","No","No","No","Internal"]
[null,null,null,23696,null,"107_17-Jan-22 21:47:48","2022-01-05T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Emergency generator MGO tank save all oily observed","Miscellaneous","General Appearance","Human Error","","","","","to be cleaned","2022-03-05T23:59:35","","Completed","2022-01-06T23:59:35","No","No","No","Internal"]
[null,null,null,23828,null,"107_2/1/2022 5:13:21 PM","2022-01-16T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Boiler Chemical Dosing Pump inoperational","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","Chemical being dosed manually.All chemical level satisfactory in boiler.","2022-03-30T23:59:35","ANTW200029","Completed","2022-12-02T23:59:35","No","No","No","Internal","will process and supply in convenient port"]
[null,null,null,23829,null,"107_2/1/2022 4:53:26 PM","2022-01-18T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Accom. AC control system, compressor and Motor Performance is abnormal","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Performance found to be sarisfactory as of now.Awaiting spare pulley for motor and compressor.","2022-03-30T23:59:35","ANTW220006, ANTW220008","Completed","2022-03-27T23:59:35","No","No","No","Internal","will process and supply in convenient port"]
[null,null,null,23830,null,"107_2/1/2022 5:22:19 PM","2022-01-20T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Aux. Cooling SW pump seal leaks. Trying to isolate for overhaul, noticed inlet valve connected to the sea chest line not holding.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Pump overhauled with the available spares.","2022-02-06T23:59:35","","Completed","2022-09-01T23:59:35","No","No","No","Internal","if the valve malfunction please order and make plan to renew. please update the pump overhaul status"]
[null,null,null,23831,null,"107_2/1/2022 5:25:13 PM","2022-01-21T23:59:35","Defect","Ship Staff","Ship Staff Insp.","#2 Boiler circulating Pump Seal leaking","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","Leak found to be very minimal.Will change with new seal when recieved.","2022-03-30T23:59:35","ANTW200029","Completed","2022-03-19T23:59:35","No","No","No","Internal","will process and supply in convenient port"]
[null,null,null,23832,null,"107_2/1/2022 5:42:41 PM","2022-01-22T23:59:35","Defect","Ship Staff","Ship Staff Insp.","ME and DG auto Back wash Filter operating mechanism not functioning on Auto","E/R - Aux. Engine,E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Backwash being carried out four times everyday manually.Pressure is satisfactory.","2022-03-30T23:59:35","ANTW220045","Completed","2022-03-27T23:59:35","No","No","No","Internal","will supply in next convenient port"]
[null,null,null,23833,null,"107_2/1/2022 5:39:17 PM","2022-01-27T23:59:35","Observation","Ship Staff","Ship Staff Insp.","#3 DG Turbocharger Gas leaking from casing Joint","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Casing Bolts and nut tighten and noticed no any leakage even at 420 kw load","2022-02-03T23:59:35","","Completed","2022-07-01T23:59:35","No","No","No","Internal","to carry out the job at anchorage and update"]
[null,null,null,23953,null,"107_2/16/2022 2:36:33 PM","2022-01-31T23:59:35","Guarantee Claim","Ship Staff","Ship Staff Insp.","#8 Hatch cover new block rec'd is leaking","Deck - Machinery","Cargo / Ballast Systems","Equipment Related","","","","","#8 Hatch cover problem solved as there was an issue with a non return valve which was installed wrongly in DD. w.r.t. New block oil flow configration to be confirmed with office assistance. If it is not matching, then we need to land this new block for replacement. One more spare block is found in the forward Bosun store, need to check and confirm its function","2022-03-30T23:59:35","ANTW215132","Completed","2022-12-02T23:59:35","No","No","No","Internal","does this confirmed by supplier to do exchanged"]
[null,null,null,23955,null,"107_2/16/2022 12:15:29 PM","2022-02-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","ECR COMPUTER CPU DEFECTIVE","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Computer used for Paper works in ECR is Defective. Showing Error code: 0x80070002 which is normally due to file corruption / registry issues. As there are Huge Paper works are being done daily & at Month end in ER, unable to manage with one computer.","2022-02-27T23:59:35","ANTW220043","Completed","2022-12-02T23:59:35","No","No","No","Internal","please seek IT to assist whether can solve the issue."]
[null,null,null,23960,null,"107_2/16/2022 3:07:07 PM","2022-02-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Steam traps in ER are not operational","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Most of the important steam trap in ER are not operational. F.O heaters of Main & Aux engine, Purifier heaters are among them. Due to this issue we are unable to maintain required temperature.","2022-03-30T23:59:35","ANTW220052","Completed","2022-10-02T23:59:35","No","No","No","Internal","will supply spare as raised RO in convenient port"]
[null,null,null,23959,null,"107_2/16/2022 2:55:52 PM","2022-02-02T23:59:35","Defect","Ship Staff","Suptd. Insp.","UMS Mode Inoperational","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","All automation related to UMS have been done.Only aux boiler level controller has to be renewed.","2022-05-29T23:59:35","ANTW220001, ANTW220045, ANTW220014","Completed","2022-03-30T23:59:35","No","No","No","Internal","will supply spare as raised RO in next convenient port"]
[null,null,null,23956,null,"107_2/16/2022 1:21:51 PM","2022-02-13T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Intermediate Shaft Bearing has slight leakage from the Aft side O-ring","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Requisition sent on 23rd Feb","2022-03-30T23:59:35","ANTW220061","Completed","2022-02-23T23:59:35","No","No","No","Internal","please reduce oil level and check if the leakage reduce. please raise RO for sealing kit if it able to renew"]
[null,null,null,23957,null,"107_2/16/2022 3:22:30 PM","2022-02-13T23:59:35","Defect","Ship Staff","Ship Staff Insp.","#2 Cyl. L.O. Pump Oil Seal Leak","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Spare pump is of wrong size.Does not fit.Have to raise Req for new pump.","2022-03-28T23:59:35","","Completed","2022-03-25T23:59:35","No","No","No","Internal","please carry out and update"]
[null,null,null,23958,null,"107_2/16/2022 3:32:54 PM","2022-02-14T23:59:35","Observation","Ship Staff","Ship Staff Insp.","#2 Prov. Ref Compr. Motor making Noise","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Vsl. has only one bearing. hence we already send requisition for Motor overhauling.","2022-03-29T23:59:35","ANTW220049","Completed","2022-02-27T23:59:35","No","No","No","Internal","will supply spare as raised RO in next convenient port"]
[null,null,null,23961,null,"107_2/16/2022 3:28:42 PM","2022-02-14T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Waste oil Sounding and DO settling tank Sounding Pipes are chocked. Improper quantity measurement.","Hull & Tanks","Eng. / Strg. Comp.","Equipment Related","","","","","Sounding pipe cleared with air and cleaning with iron rod.Now getting correct sounding.Will need to manaully clean the tank at first opportunity for good results.","2022-03-29T23:59:35","","Completed","2022-03-28T23:59:35","No","No","No","Internal","please carry out and update"]
[null,null,null,24619,null,"107_30/03/2022 15:54:24","2022-03-22T23:59:35","Defect","Ship Staff","Others (Eg. Insurance etc.)","Hot water Calorifier heating coil found defective.Low insulation.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","Heating now being done by steam.","2022-05-30T23:59:35","ANTW220071","Completed","2022-04-19T23:59:35","No","No","No","Internal","will supply the spare in next convenient port."]
[null,null,null,24963,null,"107_4/15/2022 9:04:52 PM","2022-04-03T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Aux Boiler small water leak from Water chamber into furnace.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","Water leak very small.Vessel now at sea.To be repaired at anchorage first opportunity","2022-04-21T23:59:35","","Completed","2022-04-23T23:59:35","No","No","No","Internal","the job already completed. to update"]
[null,null,null,25471,47621,"107_Tue May 31 2022 18:47:00 GMT+0800","2022-05-18T23:59:35","Breakdown,Critical Equipment","Ship Staff","Ship Staff Insp.","Emergency Generator Radiator leak","Critical Equip.","Emgcy. Systems","Equipment Related","","","","","Emergency Generator taken out of service.","2022-06-05T23:59:35","ANTW220095","Completed","2022-06-05T23:59:35","No","No","No","Internal","parts will deliver at Capetwon.pls update status for replacement"]
[null,null,null,25663,78134,"107_Mon Jun 06 2022 20:12:48 GMT+0800","2022-05-30T23:59:35","Critical Equipment","Ship Staff","Ship Staff Insp.","S-band radar unable to have stable ARPA acquisition. \nRadar no. 1 reported to have very low detection capabilities even with the correct modulation and clutter settings.","Navigation - RADAR","Navigation","Equipment Related","","","","","Request for technical assistance.","2022-06-23T23:59:35","ANT22054","Completed","2022-06-24T23:59:35","No","No","No","Internal"]
[null,null,null,23687,null,"107_17-Jan-22 21:38:47","2022-05-31T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Port bunker manifold oil spill tray drain with wood plug","Deck - Pipe / Fittings","General Appearance","Human Error","","","","","proper plug to be fabricated","2022-01-29T23:59:35","","Completed","2022-09-30T23:59:35","No","No","No","Internal"]
[null,null,null,23688,null,"107_17-Jan-22 21:40:30","2022-05-31T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Compress airline on deck leaking beside HC7 and HC4","Deck - Pipe / Fittings","General Appearance","Human Error","","","","","New line fabricated","2022-01-29T23:59:35","","Completed","2022-09-30T23:59:35","No","No","No","Internal"]
[null,null,null,23689,null,"107_17-Jan-22 21:49:31","2022-05-31T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ME LO oil cooler cooling water leakage sign observed on top flange","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Reactified","2022-06-02T23:59:35","","Completed","2022-09-30T23:59:35","No","No","No","Internal"]
[null,null,null,23690,null,"107_17-Jan-22 21:51:09","2022-05-31T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ME shaft grounding device to carry out maintenance. Slip ring to clean","E/R - Main Engine","Eng. / Strg. Comp.","Human Error","","","","","Reactified","2022-06-02T23:59:35","","Completed","2022-06-30T23:59:35","No","No","No","Internal"]
[null,null,null,23691,null,"107_17-Jan-22 21:52:43","2022-05-31T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Economizer soot blower steam drain valve leakage. Lagging to wrap properly","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Human Error","","","","","Rectified","2022-06-02T23:59:35","","Completed","2022-06-30T23:59:35","No","No","No","Internal"]
[null,null,null,23692,null,"107_17-Jan-22 21:54:45","2022-05-31T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Emergency generator both ventilator and air duct wire mesh damaged","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Human Error","","","","","changed","2022-06-02T23:59:35","","Completed","2022-06-30T23:59:35","No","No","No","Internal"]
[null,null,null,23693,null,"107_17-Jan-22 21:45:46","2022-05-31T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Both anchor chain pipe security plate excessive gap observed","Deck - Pipe / Fittings","General Appearance","Human Error","","","","","fabricated","2022-06-02T23:59:35","","Completed","2022-07-31T23:59:35","No","No","No","Internal"]
[null,null,null,23694,null,"107_17-Jan-22 21:42:33","2022-05-31T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Deck store top rusty and spot to chip and paint","Miscellaneous","General Appearance","Human Error","","","","","De rusting and painting  done","2022-01-28T23:59:35","","Completed","2022-07-31T23:59:35","No","No","No","Internal"]
[null,null,null,23480,null,"107_1/14/2022 3:41:18 PM","2022-05-31T23:59:35","Defect","Ship Staff","Ship Staff Insp.","EGE Steam inlet pipe holed","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","The whole section of pipe is been renewed","2022-01-29T23:59:35","","Completed","2022-05-31T23:59:35","No","No","No","Internal","please update on 30 Jan 2022"]
[null,null,null,30066,98745,"107_Tue Mar 14 2023 14:45:09 GMT+0800","2022-06-23T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Nav Audit / Verification","Wheel house front two window wipers are defective","Miscellaneous","Navigation","Equipment Related","","","","","Wheel house front two window wipers motors replaced, working satisfactory.","2022-07-23T23:59:35","","Completed","2022-06-26T23:59:35","No","No","No","Internal"]
[null,null,null,23481,null,"107_1/14/2022 3:31:56 PM","2022-07-31T23:59:35","Defect","Ship Staff","Ship Staff Insp.","MDO (P) level gauge is faulty","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Overhauled and fitted. ","2022-02-27T23:59:35","","Completed","2022-01-19T23:59:35","No","No","No","Internal","please keep update status"]
[null,null,null,23484,null,"107_1/15/2022 12:40:06 PM","2022-07-31T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Port cylinder LO manifold filling pipe is weakend and rusted","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","Equipment Related","","","","","New Pipe line Fabricated and fitted in place. ","2022-01-29T23:59:35","","Completed","2022-08-31T23:59:35","No","No","No","Internal","please update status and close out within the windows"]
[null,null,null,30065,88388,"107_Tue Mar 14 2023 14:37:48 GMT+0800","2022-08-29T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Nav Audit / Verification","Radio compass book is not properly filled.","Documentation","Cert. & Docu.","Human Error","","","","","Radio compass book filled properly, training conducted for importance of filling the Radio compass book.","2022-11-29T23:59:35","","Completed","2022-08-29T23:59:35","No","No","No","Internal"]
[null,null,null,27805,64383,"107_Thu Oct 20 2022 13:43:29 GMT+0800","2022-08-29T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","Engine supply Fan No.2  is in-operational due to broken impeller blades","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Inspected the fan & Motor, found all the fan blades broken from the hub. Checked the foundation of motor, found intact. Presently, Fan motor breaker is OFF and Locked out. Requistion raised for the fan. Awaiting spares. \nReceived new fan impeller on 15th Dec. at Port Suez. Installed the new impeller. Checked and replaced foundation bolts of motor, tightened with lock washers. Fan tried out, running satisfactorily.","2022-11-29T23:59:35","ANTW220163 dt. 31st Aug.2022","Completed","2022-12-17T23:59:35","No","No","No","Internal"]
[null,null,null,30070,35771,"107_Tue Mar 14 2023 17:30:24 GMT+0800","2022-10-14T23:59:35","Critical Equipment","Ship Staff","Ship Staff Insp.","Echo-sounder printing facility damaged. Cannot procure parts due to an already obsolete manufacturer model type hence suggesting total replacement of the said component.","Navigation - Echo Sounder / Speed Log","Navigation","Equipment Related","","","","","Technician boarded the vessel and replaced the whole panel which comes with a new printing facility. ","2023-02-19T23:59:35","","Completed","2023-02-19T23:59:35","No","No","No","Internal"]
[null,null,null,27806,17468,"107_Thu Nov 17 2022 23:06:26 GMT+0800","2022-10-23T23:59:35","Breakdown,Defect","Ship Staff","Ship Staff Insp.","Accommodation  A/C compressor unable to start due to defective HDD controller PCB","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","The digital display of A/C control panel is continuously flashing and there is no means of control voltage to contactors to start the system. Presently, vessel is sailing in cold area. Requisition raised for the controller PCB. Awaiting spares.\n\nReceived HD controller PCB at Port Suez on 15th Dec. 22. Replaced the HD controller with a new spare. A/C compressor test run successfully. A/C compressor put back online.","2023-01-23T23:59:35","RO – ANTW220205 ","Completed","2022-12-15T23:59:35","No","No","No","Internal",""]
[null,null,null,30077,41994,"107_Tue Mar 14 2023 17:41:24 GMT+0800","2022-10-26T23:59:35","Critical Equipment","Ship Staff","Ship Staff Insp.","Since from the commissioning of the X-band radar a power fault for relay was found for 24VDC. The fault is due to a missing terminal interconnection from ship's main output to the radar power lay terminal.","Navigation - RADAR","Navigation","Equipment Related","","","","","Electrician pathed the lay connection and trailed new supply cord from battery supply and into the overlay terminal for emergency in x-band radar. Eventually resolved the issue but after a week the issue arises again. Technician boarded the vessel in Zhoushan, China and resolved the issue.","2023-03-09T23:59:35","","Completed","2023-02-19T23:59:35","No","No","No","Internal"]
[null,null,null,27927,19247,"107_Thu Dec 08 2022 13:10:47 GMT+0800","2022-11-01T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","Aux. S.W. cooling  Pump tripped on overload. The pump shaft was hard to move, To be investigated by opening the pump for overhaul.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","","","","","The cross-over line was opened to feed sea water to the Aux. machineries. The pump was isolated for overhaul.  The impeller was disconnected from the shaft due to missing key and came in contact with the casing causing the trip.\nThe pump was then overhauled with new shaft, shaft sleeve, mechanical seal key & submerged bearings. The pump tried out and found satisfactory.","2023-01-31T23:59:35","","Completed","2022-11-05T23:59:35","No","No","No","Internal",""]
[null,null,null,30071,43889,"107_Tue Mar 14 2023 17:35:02 GMT+0800","2022-11-23T23:59:35","Critical Equipment","Ship Staff","Ship Staff Insp.","The VDR FFC lose the record feed for the DAU. Suspected bad circuit from moisture that may have ingresses the junction box for its docking module.","Navigation - VDR / BNWAS","Navigation","Equipment Related","","","","","ELCOME technician boarded the vessel in Algeciras, Spain on 5th Dec. 2022 and installed new FFC docking module which eventually resulted in the resolving of the issue.","2022-12-04T23:59:35","ANTW2022242","Completed","2022-12-04T23:59:35","No","No","No","Internal"]
[null,null,null,30069,88770,"107_Tue Mar 14 2023 17:24:31 GMT+0800","2022-12-14T23:59:35","Critical Equipment","Ship Staff","Ship Staff Insp.","X-band radar giving fault of non-video acquisition for the VDR feed. The RVI video input is absent hence giving the incomplete playback record. ","Navigation - RADAR","Navigation","Equipment Related","","","","","The technician boarded in Singapore Anchorage on Jan. 06 2023 and resolved the issue of the RVI input on VDR. ","2023-01-05T23:59:35","","Completed","2023-01-05T23:59:35","No","No","No","Internal"]
[null,null,null,28773,57658,"107_Thu Dec 22 2022 21:56:57 GMT+0800","2022-12-15T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Fresh water Generator Sea water Inlet casing for condenser damaged","Navigation - Others,E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Fresh water Generator Sea water Inlet casing for condenser replaced with new spare casing at Zhoushan DD.","2023-03-15T23:59:35","ANTW220228","Completed","2023-02-11T23:59:35","No","No","No","Internal"]
[null,null,null,28783,92307,"0_Wed Dec 28 2022 12:30:08 GMT+0800","2022-12-16T23:59:35","Non Conformity,Breakdown","Ship Staff","Ship Staff Insp.","In cross deck of #6 & #7 the fire line was found corroded and damaged underneath the angle bar support.","Deck - Pipe / Fittings","Safety / LSA / FFA","External Factors","","","","","The corroded damaged pipe line section was removed and fully new pipeline fixed. ","2023-03-16T23:59:35","","Completed","2022-12-21T23:59:35","No","No","No","Internal"]
[null,null,null,28778,38273,"107_Wed Dec 28 2022 11:54:52 GMT+0800","2022-12-25T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Inspected the 2 WBT (P) ballast tank valve and found valve seat damaged. ","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","","","",""," the 2 WBT (P) ballast tank valve seat renewed with new . boxed back and tried out, satisfactory.","2023-03-25T23:59:35","ANTW220230","Completed","2023-03-18T23:59:35","No","No","No","Internal"]
[null,null,null,28772,49843,"107_Tue Jan 10 2023 19:45:08 GMT+0800","2023-01-05T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","No.1 L.O. purifier to make operational","E/R - Purifier","Eng. / Strg. Comp.","Equipment Related","","","","","No-1 Lube oil purifier complete overhaul carried . verical shaft renewd. water block replaced with new set. all consumables renewed. electric motor overhaul carried and boxed back with new friction pads. ANTW230166 LO Purifier- air filter with solenoid valve SV4 complete assembly received at Singapore on 28-June-2023. Same Fitted and No.1 LO Purifier tried out, working satisfactory.","2023-02-05T23:59:35","","Completed","2023-06-30T23:59:35","No","No","No","Internal"]
[null,null,null,28774,53004,"107_Tue Jan 10 2023 20:08:19 GMT+0800","2023-01-05T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Aux. engine No.3 funnel corroded, to make DD spec. ","E/R - Aux. Engine,E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","DD specs were made and repairs on the AE-3 corroded funnels are carried in Zhoushan DD by shore workshop. ","2023-01-12T23:59:35","","Completed","2023-02-26T23:59:35","No","No","No","Internal"]
[null,null,null,28775,26934,"107_Tue Jan 10 2023 19:52:47 GMT+0800","2023-01-05T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","M/E Viscosity control valve to make operational","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","diaphragms renewed on 11-Apr-2023. tested with air, operating satisfactory.","2023-02-05T23:59:35","ANTW230005","Completed","2023-04-12T23:59:35","No","No","No","Internal"]
[null,null,null,28776,35940,"107_Tue Jan 10 2023 19:38:15 GMT+0800","2023-01-05T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","SW pipe for reefer cooling system on top of purifier room to renew due to leakage observed.","E/R - Aux. Mach.,E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","SW pipe for reefer cooling system on top of purifier room replaced with new fabricated pipes.","2023-01-26T23:59:35","","Completed","2023-02-25T23:59:35","No","No","No","Internal"]
[null,null,null,28777,91438,"107_Tue Jan 10 2023 19:31:06 GMT+0800","2023-01-05T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Steering gear ram seal to check clearance and rectify leakage.","Navigation - Others,E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Ram seals are renewed by shore technicians during Steering gear servicing.","2023-01-26T23:59:35","","Completed","2023-03-29T23:59:35","No","No","No","Internal"]
[null,null,null,28779,97183,"107_Tue Jan 10 2023 19:59:34 GMT+0800","2023-01-05T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Cascade tank level guage glass broken","Hull & Tanks","Eng. / Strg. Comp.","Equipment Related","","","","","broken gauge glass renewed.","2023-01-12T23:59:35","","Completed","2023-03-31T23:59:35","No","No","No","Internal"]
[null,null,null,28780,14877,"107_Tue Jan 10 2023 19:47:07 GMT+0800","2023-01-05T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","No.1 HFO purifier to make operational","E/R - Purifier","Eng. / Strg. Comp.","Equipment Related","","","","","FO Purifier-1 leakage monitor settings were not set in accordance to the maker’s manual. Also, the back-pressure adjusting valve was fully open causing more time to built the pressure, same is adjusted. The FO Purifier no-1 tried out after these adjustments and tried out for 4 hrs. manual desludging carried several times and it came on feed without triggering shutdown cycle.","2023-02-05T23:59:35","","Completed","2023-04-15T23:59:35","No","No","No","Internal"]
[null,null,null,28781,42935,"107_Tue Jan 10 2023 20:05:33 GMT+0800","2023-01-05T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Pressure and Temperature calibrators to calibrate ashore annually","Documentation","Eng. / Strg. Comp.","Equipment Related","","","","","sent ashore as per office instructions. calibration certificates received, same updated in PAL","2023-02-05T23:59:35","","Completed","2023-04-03T23:59:35","No","No","No","Internal"]
[null,null,null,28782,39593,"107_Tue Jan 10 2023 19:23:30 GMT+0800","2023-01-05T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","\nE/R workshop fire protective curtain to order and replace.\n\n\n","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","E/R workshop fire protective curtain replaced.","2023-02-05T23:59:35","ANTW230020","Completed","2023-03-23T23:59:35","No","No","No","Internal"]
[null,null,null,28784,71608,"107_Tue Jan 10 2023 19:43:08 GMT+0800","2023-01-05T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","No.2 A/E New cooling water pipe leaking sign observed to check","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","PIPE DISMANTLED.FLANGES CLEANED.GASKETS REPLACED.LEAKAGE RECTIFIED.",null,"","Completed","2023-01-10T23:59:35","No","No","No","Internal"]
[null,null,null,28785,29865,"107_Tue Jan 10 2023 19:33:41 GMT+0800","2023-01-05T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","A/E fuel oil supply and cirucualting pump underneath to clean and paint","Navigation - Echo Sounder / Speed Log,E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","","","","","A/E fuel oil supply and circulating pump & M/E fuel oil supply and circulating pump underneath tray spaces cleaned and painted.","2023-01-12T23:59:35","","Completed","2023-01-10T23:59:35","No","No","No","Internal"]
[null,null,null,28786,89361,"107_Tue Jan 10 2023 19:55:17 GMT+0800","2023-01-05T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Cascade tank minor oil observed , to remove throughly","Hull & Tanks","Eng. / Strg. Comp.","Equipment Related","","","","","OIL CLEANED.","2023-01-12T23:59:35","","Completed",null,"No","No","No","Internal"]
[null,null,null,28787,98503,"107_Tue Jan 10 2023 19:35:46 GMT+0800","2023-01-05T23:59:35","Defect,Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","3 sets of A/E underneath to clean up","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","ALL 3 AUX ENGINE UNDER SPACES CLEANED UP AND PAINTED AS REQUIRED.","2023-01-12T23:59:35","","Completed",null,"No","No","No","Internal"]
[null,null,null,28788,64237,"107_Tue Jan 10 2023 19:28:34 GMT+0800","2023-01-05T23:59:35","Defect,Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Waste stores/Materials to dispose from Engine store room ","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","WASTE MATERIALS SUITABLY DISPOSED / INCINERATED.","2023-01-19T23:59:35","","Completed",null,"No","No","No","Internal"]
[null,null,null,28789,12359,"107_Tue Jan 10 2023 19:41:08 GMT+0800","2023-01-05T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Boiler auto filling valve to rectify leakage of valve spindle","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","LEAKAGE RECTIFIED.","2023-02-15T23:59:35","","Completed",null,"No","No","No","Internal"]
[null,null,null,28791,47604,"107_Tue Jan 10 2023 19:57:48 GMT+0800","2023-01-05T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Cascade tank temperature to maintain 80 deg.C,  observed 60 deg. C while inspection.","Hull & Tanks","Eng. / Strg. Comp.","Equipment Related","","","","","Opened Condenser by-pass to maintain 80 deg. C.",null,"","Completed","2023-01-06T23:59:35","No","No","No","Internal"]
[null,null,null,28790,42034,"107_Tue Jan 24 2023 06:27:10 GMT+0800","2023-01-08T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Portside anchor wash line was found choke.","Deck - Pipe / Fittings","ISM Related","Equipment Related","","","","","The pipeline was removed and the choked pipe was cleared.","2023-04-07T23:59:35","","Completed","2023-01-13T23:59:35","No","No","No","Internal"]
[null,null,null,30067,75049,"107_Tue Mar 14 2023 17:13:49 GMT+0800","2023-02-07T23:59:35","Critical Equipment","Ship Staff","Ship Staff Insp.","The VDR displayed the Main Engine Module alarm which was a result of the then defective alarm monitoring system. It was never cancelled, even if attempted to and will persist until the defect in the alarm system is resolved. ","Navigation - VDR / BNWAS","Navigation","Equipment Related","","","","","A Konsberg-accredited technician boarded the vessel in Zhoushan, China and found the fault and thereafter resolved it.","2023-02-28T23:59:35","","Completed","2023-03-13T23:59:35","No","No","No","Internal"]
[null,null,null,30072,86961,"107_Wed Mar 15 2023 16:05:43 GMT+0800","2023-02-07T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Bosun store skylight cover retention channel found wasted. ","Hull & Tanks","Structural Condn. / WT integrity ","Equipment Related","","","","","Retention channel renewed and new rubber packing installed.","2023-05-06T23:59:35","","Completed","2023-02-23T23:59:35","No","No","No","Internal"]
[null,null,null,30061,36639,"107_Tue Mar 14 2023 13:57:51 GMT+0800","2023-02-13T23:59:35","Observation","Owner / Marine / Tech. Suptd.","ISM Audit","Insulation in various position found oil soaked and painting, need to replace","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","the oil soaked insulations are removed and new insulation material fitted on pipings.","2023-03-30T23:59:35","","Completed","2023-03-09T23:59:35","No","No","No","Internal"]
[null,null,null,30062,68435,"0_Tue Mar 14 2023 14:01:24 GMT+0800","2023-02-13T23:59:35","Observation","Ship Staff","ISM Audit","Sounding pipe found pressure drain device found clogged.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Industry Issue,Equipment Related","","","","","the sounding pipe pressure drain valves renewed with new ones.","2023-03-30T23:59:35","","Completed","2023-03-11T23:59:35","No","No","No","Internal"]
[null,null,null,30063,82012,"0_Tue Mar 14 2023 14:04:50 GMT+0800","2023-02-13T23:59:35","Observation","Ship Staff","ISM Audit","The A-60 insulation door of emergency escape trunk frame found oil soaked.","Miscellaneous","Eng. / Strg. Comp.","Inappropriate Procedure","","","","","the oil soaked insulation replaced with new insulation sheet.","2023-03-30T23:59:35","","Completed","2023-03-11T23:59:35","No","No","No","Internal"]
[null,null,null,30064,36258,"0_Tue Mar 14 2023 14:07:27 GMT+0800","2023-02-13T23:59:35","Observation","Ship Staff","ISM Audit","ECR AC unit return air vent louvers found damaged, to repair or replace","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","the damaged louvers are replaced with new louver set.","2023-03-30T23:59:35","","Completed","2023-03-10T23:59:35","No","No","No","Internal"]
[null,null,null,30068,81621,"0_Tue Mar 14 2023 14:09:59 GMT+0800","2023-02-13T23:59:35","Observation","Ship Staff","ISM Audit","One Emergency light casing on poop deck Port found wasted","Miscellaneous","General Appearance","Equipment Related","","","","","Emergency light casing on poop deck Port replaced with new spare.","2023-03-30T23:59:35","","Completed","2023-03-04T23:59:35","No","No","No","Internal"]
[null,null,null,30080,41538,"107_Mon Apr 10 2023 14:22:33 GMT+0800","2023-03-19T23:59:35","Defect","Ship Staff","Ship Staff Insp.","When hoisting wires of bunker davit(P&S) were removed from the wire drum for wire renewal work, wire drums were found corroded and wasted.","Deck - Machinery","Safety / LSA / FFA","Equipment Related","","","","","Referred shipyard to repair and fabricate wasted wire drum.  Repaired work has done by the shipyard and new wire installed on the drum of bunker davit(P&S).","2023-06-19T23:59:35","","Completed","2023-03-31T23:59:35","No","No","No","Internal"]
[null,null,null,30082,50950,"107_Mon Apr 10 2023 14:39:04 GMT+0800","2023-03-19T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Anchor washing pipes on the anchor hawse pipes(P&S) were found leakage.","Deck - Mooring Machinery","Mooring","Equipment Related","","","","","Referred shipyard to repair leakage of anchor washing pipes(P&S). After repaired work, tested running of anchor wash water. No leakage was found.","2023-06-19T23:59:35","","Completed","2023-03-29T23:59:35","No","No","No","Internal"]
[null,null,null,30081,44173,"107_Mon Apr 10 2023 14:31:10 GMT+0800","2023-03-21T23:59:35","Defect","Ship Staff","Ship Staff Insp.","When wire was removed from the wire drum of lifeboat davit(P) for wire renewal,  the wire drum was found corroded and wasted.","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","Referred shipyard to fabricate and repair the wasted wire drum. After shipyard has repaired, install new wire on the drum and tested operation of lifeboat davit(P). Found satisfactory.","2023-06-21T23:59:35","","Completed","2023-03-29T23:59:35","No","No","No","Internal"]
[null,null,null,30087,25415,"107_Mon Apr 10 2023 15:01:11 GMT+0800","2023-03-21T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Found several leakage points on deck fire main lines due to corrosion and worn down of the pipes and joints.","Deck - Pipe / Fittings","Safety / LSA / FFA","Equipment Related","","","","","Referred shipyard to replaced damaged and leakage parts of fire main line. Shipyard has done the job and tested running of fire pump. No leakage were found and satisfactory.","2023-06-21T23:59:35","","Completed","2023-03-29T23:59:35","No","No","No","Internal"]
[null,null,null,30079,27373,"107_Mon Apr 10 2023 14:11:06 GMT+0800","2023-03-23T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Porthole glass in CCR was cracked.","Accommodation","Structural Condn. / WT integrity ","Equipment Related","","","","","Raised requisition for new porthole glass and replaced the cracked glass with new glass.","2023-06-23T23:59:35","","Completed","2023-04-04T23:59:35","No","No","No","Internal"]
[null,null,null,30084,70472,"107_Mon Apr 10 2023 15:05:33 GMT+0800","2023-03-23T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Embarkation ladders for liferaft (3nos) were found aged and worn down on the side ropes.","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","Raised requisition for new embarkation ladders.  Damaged ladders were disposed to the shore and new embarkation ladders put in the respective location.","2023-06-23T23:59:35","","Completed","2023-03-29T23:59:35","No","No","No","Internal"]
[null,null,null,30083,34328,"107_Mon Apr 10 2023 14:54:11 GMT+0800","2023-03-27T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Rubber packings of hatch cover natural vent covers were found damaged, retention channels for rubber packing were corroded and worn down.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","Raised requisition for new rubber packings. Fabricated new retention channel for rubber packings. Installed new rubber packings and boxed back all the hatch cover natural vent covers.","2023-06-27T23:59:35","","Completed","2023-04-08T23:59:35","No","No","No","Internal"]
[null,null,null,30086,38754,"107_Sat Apr 08 2023 16:43:25 GMT+0800","2023-03-29T23:59:35","Defect","Ship Staff","Ship Staff Insp.","10nos of immersion suits found defect during air-pressure test carried out by shore technician and ship staff.","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","defective immersion suits are replaced with newly received spare immersion suits","2023-06-29T23:59:35","","Completed","2023-04-10T23:59:35","No","No","No","Internal"]
[null,null,null,30089,57423,"107_Sat Apr 08 2023 16:26:04 GMT+0800","2023-03-29T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Manual handles for lifeboat davit winch (p&s) were found wasted and difficult to operate.","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","New manual handles for lifeboat davit winch(2nos) have received and tested operation. Found satisfactory.","2023-06-29T23:59:35","","Completed","2023-04-12T23:59:35","No","No","No","Internal"]
[null,null,null,30094,39964,"107_Mon Apr 10 2023 14:48:27 GMT+0800","2023-03-29T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Several Ballast tank air vent heads were found damaged and defects. 10 pcs of vent head were fully corroded and need to be replaced with new. 5pcs of float discs were cracked and all vent head rubber packings were damaged.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","","","","","10pcs of vent head were replaced with new vent heads by shipyard. 2pcs of vent head was replaced by ship crew. Damaged float discs and rubber packing replacement work has been done by ship crew. Fabricated damaged vent head covers by ship crew and boxed back. ","2023-06-29T23:59:35","","Completed","2023-04-26T23:59:35","No","No","No","Internal"]
[null,null,null,30078,10864,"107_Thu Apr 06 2023 10:41:29 GMT+0800","2023-03-30T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Lifeboat davit winch(P) ratchet bearing is not holding.","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","work in progress by shore technicians at Zhoushan DD.","2023-06-29T23:59:35","","Completed","2023-04-06T23:59:35","No","No","No","Internal"]
[null,null,null,30076,87195,"107_Sat Apr 08 2023 16:52:00 GMT+0800","2023-03-31T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Testing of de-watering system was carried out and found out that water cannot pump out from bosun store bilge well.","Deck - Pipe / Fittings","Emgcy. Systems","Equipment Related","","","","","Checked manual and remote valves open/closed condition and found that valves are operating properly. Dismantle de-watering eductor and related fittings. Found out that eductor was choke by mud due to ship was laying at muddy water areas. Thoroughly cleaned the eductor  and boxed back.  \nTested de-watering system and found satisfactory.","2023-05-29T23:59:35","","Completed","2023-04-01T23:59:35","No","No","No","Internal"]
[null,null,null,30073,67636,"107_Tue Apr 04 2023 08:28:10 GMT+0800","2023-04-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","AE FO QCV valves are sluggish in operation, air leakage from the pneumatic cylinder.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","defective QCV overhauled with new O-rings. system tested and found satisfactory.","2023-06-30T23:59:35","","Completed","2023-04-01T23:59:35","No","No","No","Internal"]
[null,null,null,30074,81841,"0_Tue Apr 04 2023 08:30:53 GMT+0800","2023-04-02T23:59:35","Defect","Ship Staff","Ship Staff Insp.","2 nos FO tanks QCV found sluggish in operation and 1 QCV for DO service tanks is not operable.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","the QCV overhauled with new O-rings and tried out satisfactorily.\nDO tanks QCV overhauled and the air pipe clogging cleared. operated and found working satisfactory.","2023-07-01T23:59:35","","Completed","2023-04-02T23:59:35","No","No","No","Internal"]
[null,null,null,30075,38564,"107_Thu Apr 06 2023 10:46:05 GMT+0800","2023-04-02T23:59:35","Defect","Ship Staff","Ship Staff Insp.","the QCV for 3 FO tanks were found to be sluggish in operation.","E/R - Pipes/ valves & fittings","Safety / LSA / FFA","Equipment Related","","","","","the QCV isolated and dismantled, O-rings are found brittle, same renewed. Cylinder found to be with scaling, same cleaned.one of the QCV's air supply line was clogged at bend. line clogging cleared. system valves tried out, working satisfactory.","2023-07-02T23:59:35","","Completed","2023-04-02T23:59:35","No","No","No","Internal"]
[null,null,null,30085,29385,"107_Sat Apr 08 2023 16:20:28 GMT+0800","2023-04-02T23:59:35","Critical Equipment","Ship Staff","Ship Staff Insp.","- 02 NOS. PILOT ROPE LADDERS 11mtr (P&S) - FOUND DAMAGED.\n- 01 NO. PILOT ROPE LADDER 9mtr - AGED AND CHOKE CLAMPS LOOSENED.","Critical Equip.","Safety / LSA / FFA","Equipment Related","","","","","RO received and defective pilot ladders are replaced with newly received pilot ladders","2023-07-02T23:59:35","","Completed","2023-04-09T23:59:35","No","No","No","Internal"]
[null,null,null,30091,87696,"107_Thu Apr 13 2023 18:16:21 GMT+0800","2023-04-12T23:59:35","Defect","Ship Staff","Ship Staff Insp.","the safety cap of Main Engine bursting disc was observed to be not free in operation due to excessive paint and deposits in between saety cap and perforated disc.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Main Engine all units safety cap assy removed and same freed, bursting discs renewed. operation for blocking the safety cap checjked and found to be operating with ease. ","2023-07-12T23:59:35","","Completed","2023-04-12T23:59:35","No","No","No","Internal"]
[null,null,null,30092,43774,"107_Sat Apr 15 2023 14:54:34 GMT+0800","2023-04-12T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Main Engine unit-1 fuel pump puncture valve leaking due to defective/ brittle O-ring.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Main Engine unit-1 fuel pump puncture valve removed , tested and fitted back with new O-rings. leak rectified.","2023-07-13T23:59:35","","Completed","2023-04-13T23:59:35","No","No","No","Internal"]
[null,null,null,31037,10195,"0_Mon Jul 03 2023 17:54:04 GMT+0800","2023-04-14T23:59:35","Critical Equipment","Ship Staff","Ship Staff Insp.","Emergency Generator Cooling Water Pump casing found crack,  temporary repaired. Need Renewal.","Critical Equip.","Emgcy. Systems","Equipment Related","","","","","Emergency Generator Cooling Water Pump temporary repaired Cracked casing replaced with new casing, bearing, axial face seal and impeller. gasket renewed. Anti freeze added in the radiator with 40:60 ratio as per maker's manual.\nemergency generator engine tried out with battery start and hydraulic starter, found operating satisfactory.\nno leak observed from tale tell hole of water pump casing.","2023-07-14T23:59:35","","Completed","2023-07-02T23:59:35","No","No","No","Internal"]
[null,null,null,30088,69522,"0_Sat Apr 15 2023 14:57:53 GMT+0800","2023-04-14T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Aux. Engine no-1 exhaust gas leaking from exhaust manifold due to ruptured gasket.","E/R - Aux. Engine,E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Aux. Engine no-1 exhaust manifold's ruptured gasket replaced and leak rectified.","2023-07-14T23:59:35","","Completed","2023-04-14T23:59:35","No","No","No","Internal"]
[null,null,null,30090,63952,"107_Thu May 04 2023 12:39:03 GMT+0800","2023-04-22T23:59:35","Observation","Ship Staff","Ship Staff Insp.","ME Unit-1 fwd injector slightly leaking from the sealing area during operation.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","the defective fuel injector replaced with overhauled and pressure tested one.","2023-07-24T23:59:35","","Completed","2023-04-24T23:59:35","No","No","No","Internal"]
[null,null,null,30093,42810,"0_Thu May 04 2023 12:41:52 GMT+0800","2023-04-23T23:59:35","Observation","Ship Staff","Ship Staff Insp.","ME Unit-2 fuel pump deflector area having small oil trace, suspected leak due to eroded deflector or damaged seal ring.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","the deflector removed and observed to be eroded, same renewed with new spare deflector and seal ring.","2023-07-23T23:59:35","","Completed","2023-04-24T23:59:35","No","No","No","Internal"]
[null,null,null,30060,71806,"107_Thu May 04 2023 12:53:42 GMT+0800","2023-05-02T23:59:35","Defect","Ship Staff","Ship Staff Insp.","duct keel fwd suction line to the cargo hold bilge stripping line having leak in piping.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","","","","","the wasted out pipe branch renewed and tested.","2023-08-03T23:59:35","","Completed","2023-05-15T23:59:35","No","No","No","Internal"]
[null,null,null,30095,67743,"107_Sun May 07 2023 10:59:26 GMT+0800","2023-05-05T23:59:35","Defect","Ship Staff","Ship Staff Insp.","ECR AC unit's condenser cooling sea water inlet line stub is wasted out and started leaking.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","-ECR AC unit's condenser cooling sea water inlet line leaky stub replaced with newly fabricated pipe stub. system tried out, found working satisfactory . leak rectified.","2023-08-05T23:59:35","","Completed","2023-05-05T23:59:35","No","No","No","Internal"]
[null,null,null,30097,31123,"107_Mon May 15 2023 00:10:52 GMT+0800","2023-05-08T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Sea water leaking from No. 1  Ballast pump neck bearing cover. Cover removed and found pin hole.","Cargo Mach.,E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","","","","","No. 1  Ballast pump neck bearing cover removed from in place and repair work carried out. leak rectified.","2023-08-08T23:59:35","","Completed","2023-05-08T23:59:35","No","No","No","Internal"]
[null,null,null,30096,42857,"107_Sun May 14 2023 23:26:05 GMT+0800","2023-05-09T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Oil leaking from hydraulic valve actuator (valve-110) block.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Hydraulic Valve actuator mounting block removed and O - rings found brittle, same renewed. System tried out,  found working satisfactory.  Leakage rectified.","2023-08-09T23:59:35","","Completed","2023-05-09T23:59:35","No","No","No","Internal"]
[null,null,null,31023,62953,"107_Thu Jun 01 2023 19:54:28 GMT+0800","2023-05-15T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Forward spring winch hydraulic line leaking from the square flange due to failure of fastener.","Deck - Pipe / Fittings","Mooring","Equipment Related","","","","","the pipe removed after isolating the hydraulic system, O-rings at both end rebnewed and the new fasteners are used while assemblying as the old fitted fasteners were observed to be of poor quality/ wrong size combinations. sytem tried out and found to be satisfactory without leakage.","2023-05-16T23:59:35","","Completed","2023-05-16T23:59:35","No","No","No","Internal"]
[null,null,null,30098,64613,"107_Sat May 20 2023 18:36:05 GMT+0800","2023-05-15T23:59:35","Observation","Ship Staff","Ship Staff Insp.","oil leaking observed in the remote operated valve (BS-017) for duct keel fwd suction.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","","","","","Valve block removed ind inspected, O-rings are found to be thinned and same renewed and valve block assembled. tried out for operation. working satisfactory without leakage.","2023-08-15T23:59:35","","Completed","2023-05-15T23:59:35","No","No","No","Internal"]
[null,null,null,31021,51643,"107_Tue May 23 2023 14:45:56 GMT+0800","2023-05-21T23:59:35","Observation","Ship Staff","Ship Staff Insp.","the hydraulic oil minor leakage observed at forward spring winch operating lever during operation.","Deck - Mooring Machinery","Mooring","Equipment Related","","","","","the spring winch isolated and operating lever removed from location, found O-rings were thinned down and unable to seal. same renewed and boxed back. system tried out. working satisfactory. leak rectified.","2023-08-21T23:59:35","","Completed","2023-05-21T23:59:35","No","No","No","Internal"]
[null,null,null,31022,69381,"0_Tue May 23 2023 14:49:02 GMT+0800","2023-05-21T23:59:35","Observation","Ship Staff","Ship Staff Insp.","minor oil leak observed during operation from windlass valve block .","Deck - Mooring Machinery","Mooring","Equipment Related","","","","","the windlass isolated and valve block removed from location, found O-rings were thinned down and unable to seal. same renewed and boxed back. system tried out. working satisfactory. leak rectified.","2023-08-21T23:59:35","","Completed","2023-05-21T23:59:35","No","No","No","Internal"]
[null,null,null,31024,47304,"107_Thu Jun 01 2023 18:01:31 GMT+0800","2023-05-31T23:59:35","Defect","Ship Staff","Ship Staff Insp.","One bottom frame of midship pilot assist ladder (stbd ) few rivets are observed to be detached.","Miscellaneous","Safety / LSA / FFA","Equipment Related","","","","","Fixed back new rivets on the loose bottom frame of midship pilot assist ladder (stbd) and found satisfactory.","2023-06-04T23:59:35","","Completed","2023-06-02T23:59:35","No","No","No","Internal"]
[null,null,null,31025,26656,"107_Thu Jun 01 2023 17:45:04 GMT+0800","2023-05-31T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Stepping  plate to the entrance of tally office observed to be appreciably wasted out and need renewal. ","Deck - Pipe / Fittings","Safety / LSA / FFA","Equipment Related","","","","","Cut off wasted stepping plate and side supports. Fabricated and welded new stepping plate and side supports. Applied paint on new stepping plate, side supports and welding seams. Found satisfactory.\n","2023-06-04T23:59:35","","Completed","2023-06-03T23:59:35","No","No","No","Internal"]
[null,null,null,31035,47954,"107_Fri Jun 09 2023 15:08:31 GMT+0800","2023-06-07T23:59:35","Defect","Ship Staff","Ship Staff Insp.","ME jacket fresh water cooler sea water inlet line reducer leaking from weld seam","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","ME jacket fresh water cooler sea water inlet line reducer replaced with new fabricated spare reducer.","2023-09-07T23:59:35","","Completed","2023-07-30T23:59:35","No","No","No","Internal"]
[null,null,null,31026,56600,"107_Thu Jun 15 2023 21:17:46 GMT+0800","2023-06-10T23:59:35","Defect","Ship Staff","Ship Staff Insp.","ER Workshop 440V welding machine showing low insulation.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","replaced with new welding machine","2023-09-09T23:59:35","","Completed","2023-06-27T23:59:35","No","No","No","Internal"]
[null,null,null,31034,25114,"107_Sat Jul 15 2023 13:55:19 GMT+0800","2023-06-14T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Lifeboat remote release wire pulleys support bars on both side of lifeboat (Port & stbd) were found wasted due to corrosion.","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","Fabricated new support bars in engine room workshop. Requested office concurrence for hot work permit. Chopped off wasted support bars and welded newly fabricated support bars. Notified office after work completion.","2023-09-13T23:59:35","","Completed","2023-07-09T23:59:35","No","No","No","Internal"]
[null,null,null,31032,91141,"107_Sat Jul 15 2023 13:39:38 GMT+0800","2023-06-23T23:59:35","Defect","Ship Staff","Ship Staff Insp.","5 steps of forecastle store entrance ladder found weak and thinned down due to corrosion.","Deck - Pipe / Fittings","Safety / LSA / FFA","Equipment Related","","","","","Fabricated new ladder steps in engine room work shop. Requested office concurrence for hot work and work aloft permit. Chopped off thinned down steps and welded new steps in forecastle store entrance ladder. Notified office after job completion.","2023-09-22T23:59:35","","Completed","2023-07-09T23:59:35","No","No","No","Internal"]
[null,null,null,31029,84841,"107_Fri Jun 30 2023 13:33:36 GMT+0800","2023-06-26T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Hospital space EVAC toilet system water valve is leaking internally, need replacement","Accommodation","MLC Related","Equipment Related","","","","","the defective EVAC system water valve replaced and system tried out, satisfactory.","2023-07-29T23:59:35","","Completed","2023-06-26T23:59:35","No","No","No","Internal"]
[null,null,null,31028,99729,"107_Fri Jun 30 2023 13:18:50 GMT+0800","2023-06-27T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","lifeboat davit gear box sight glass covered with paint","Deck - Machinery","General Appearance","Human Error","","","","","sight glass paint removed and crew briefed about the same","2023-06-27T23:59:35","","Completed","2023-06-27T23:59:35","No","No","No","Internal"]
[null,null,null,31036,96935,"107_Fri Jun 30 2023 13:25:18 GMT+0800","2023-06-27T23:59:35","Observation","Ship Staff","Ship Staff Insp.","ME unit-6 fuel pump's fuel  inlet pipe small portion is not covered properly with lagging ","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","lagging put properly and the bare pipe is insulated to avoid potential injury .","2023-07-26T23:59:35","","Completed","2023-06-27T23:59:35","No","No","No","Internal"]
[null,null,null,31038,77727,"107_Fri Jun 30 2023 13:22:27 GMT+0800","2023-06-27T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","embarkation ladder secured from thin frame, proper pad eye to be fabricated at both sides.","Miscellaneous","Safety / LSA / FFA","Equipment Related","","","","","Fabricated 2 pairs of strong pad eyes and welded on the lifeboat deck (port & stbd) for securing of embarkation ladders.","2023-07-27T23:59:35","","Completed","2023-07-02T23:59:35","No","No","No","Internal"]
[null,null,null,31040,66666,"107_Mon Jul 03 2023 17:47:20 GMT+0800","2023-06-27T23:59:35","Critical Equipment","Owner / Marine / Tech. Suptd.","Suptd. Insp.","'Lifeboat Port davit gear box broken sight glass need renewal","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","'Lifeboat Port davit gear box broken sight glass renewed. Gear box cover opened up and inspected. Gear oil topped up.","2023-07-27T23:59:35","","Completed","2023-07-02T23:59:35","No","No","No","Internal"]
[null,null,null,31027,51100,"107_Fri Jun 30 2023 13:12:10 GMT+0800","2023-06-28T23:59:35","Other","Ship Staff","Ship Staff Insp.","low insulation alarm activated at start of the MAC no-1","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related","","","","","MAC-1 isolated and terminal box inspected, observed wire sheathing is damaged and conductors tiuching the unction box casing. same rectified by putting heat shrinks on bare conductor. boxed back and tried out, satisfactory.","2023-09-28T23:59:35","","Completed","2023-06-28T23:59:35","No","No","No","Internal"]
[null,null,null,31039,48601,"0_Mon Jul 03 2023 17:51:43 GMT+0800","2023-06-30T23:59:35","Critical Equipment","Ship Staff","Ship Staff Insp.","Hydraulic starter pressure gauge found defective, need renewal.","Critical Equip.","Emgcy. Systems","Equipment Related","","","","","hydraulic starter pressure gauge was defective, same renewed.  EMDG tried out working satisfactory.","2023-07-09T23:59:35","","Completed","2023-07-02T23:59:35","No","No","No","Internal"]
[null,null,null,31041,30701,"107_Sat Jul 15 2023 11:21:07 GMT+0800","2023-07-05T23:59:35","Defect","Ship Staff","Ship Staff Insp.","during ME scavenge space inspection, ME unit-5 observed to have water on piston crown top. suspected leakge from cylinder cover","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","ME unit-5 cylinder cover removed and pressure tested, found water leaking in combustion side. ME cylinder cover replaced with spare one with new O-rings. pressure tested and fitted back in unit-5. ME tried out working satisfactory. ME unit-5 under piston inspection carried on 08-Jul-2023, found satisfactory with no leakages.","2023-07-14T23:59:35","","Completed","2023-07-07T23:59:35","No","No","No","Internal"]
[null,null,null,31033,31311,"107_Sat Jul 15 2023 13:45:54 GMT+0800","2023-07-09T23:59:35","Defect","Ship Staff","Ship Staff Insp.","It was observed that door hinge, rubber packing retention channel, locking eye and door opener holder of battery room weathertight door were wasted and thinned down due to corrosion.","Accommodation","General Appearance","Equipment Related","","","","","Fabricated door hinges, locking eye and door opener holder were fabricated in engine room workshop. Requested office concurrence for hot work permit. Chopped of wasted sections and welded newly fabricated items. Notified office after work completion.","2023-10-08T23:59:35","","Completed","2023-07-11T23:59:35","No","No","No","Internal"]
[null,null,null,31030,46654,"0_Sat Jul 15 2023 11:24:15 GMT+0800","2023-07-12T23:59:35","Defect","Ship Staff","Ship Staff Insp.","AE-1 Engine RPM tachometer observed to showing wrong RPM, need renewal.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","AE-1 Engine RPM tachometer replaced with new spare, engine tried out and observed to be working satisfactory.","2023-10-12T23:59:35","","Completed","2023-07-12T23:59:35","No","No","No","Internal"]
[null,null,null,31031,59786,"0_Sat Jul 15 2023 11:27:04 GMT+0800","2023-07-13T23:59:35","Defect","Ship Staff","Ship Staff Insp.","during Weekly routine starting of Emergency Generator by hydraulic means, observed Hydraulic Hand pump unable to develop pressure more than 100 bar. Suspected air in the system or defective sealing","Critical Equip.","Safety / LSA / FFA","Equipment Related","","","","","Air venting carried as per maker’s manual procedure, and tried out with no improvement in developed pressure.\nHydraulic Hand pump immediately replaced with spare hydraulic Hand pump, tried out with hydraulic starter. Working satisfactory\n","2023-07-14T23:59:35","","Completed","2023-07-13T23:59:35","No","No","No","Internal"]
[null,null,null,31157,47968,"107_Thu Aug 10 2023 12:26:11 GMT+0800","2023-08-09T23:59:35","Observation","Ship Staff","Ship Staff Insp.","No proper insulation of the exhause pipe between the exhaust manifold and turbocharger of all AEs.","E/R - Aux. Engine","ISM Related","Equipment Related","","","","","Turbocharger inlet pipes of all AE covered with new insulation. ","2023-09-09T23:59:35","","Completed","2023-08-13T23:59:35","No","No","No","Internal"]
[null,null,null,null,26373,"107_Fri Jun 30 2023 13:16:46 GMT+0800","2023-06-27T08:00:00","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","engine room bottom platform floor plate's counter sunk screws are missing","Miscellaneous","Eng. / Strg. Comp.","Inappropriate Procedure","","","","","Counter sunk screws are received at Singapore and the fixing job of the E/R bottom floor plates is completed","2023-08-30T08:00:00","ANTW230195- ER STORE- SEA WATER PIPE LINE REPAIRS","Completed","2023-08-18T08:00:00","No","No","No","Internal"]
[null,null,null,null,54541,"107_Tue Aug 15 2023 18:38:52 GMT+0800","2023-08-14T08:00:00","Defect","Ship Staff","Ship Staff Insp.","On deck fire main line was found leaked near No. 5 cargo hold.","Deck - Pipe / Fittings","Emgcy. Systems","External Factors","","","","","Fire main line pipe  (125A )  8 Meters renewed. Found no leaks.","2023-08-30T08:00:00","","Completed","2023-08-17T08:00:00","No","No","No","Internal"]
[null,null,null,null,46218,"107_Thu Aug 31 2023 17:31:11 GMT+0800","2023-08-21T08:00:00","Observation","Ship Staff","Ship Staff Insp.","All ER bilge wells found untidy. Gratings found corroded","E/R - Pipes/ valves & fittings","General Appearance","External Factors","","","","","Bilge wells cleaned, de-mugged  and painted in light colour. Gratings de-rusted and painted.","2023-09-15T08:00:00","","Completed","2023-08-23T08:00:00","No","No","No","Internal"]
[null,null,null,null,64581,"107_Fri Sep 01 2023 01:28:48 GMT+0800","2023-08-18T08:00:00","Defect","Ship Staff","Ship Staff Insp.","During Routine Rounds The Forecastle Fire Line Pressure Gauge Was Found Defective With The Wheel For Operating The Valve Sheared Off.","Deck - Pipe / Fittings,LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","Immediately The Faulty Pressure Gauge And Complete Valve Was Renewed With The Spares Onboard And Confirmed Working On Running The Fire Pump.","2023-08-19T08:00:00","","Completed","2023-08-19T08:00:00","No","No","No","Internal"]
[null,null,null,null,42041,"107_Fri Sep 01 2023 16:02:18 GMT+0800","2023-08-16T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Cross over bridge chequer plate found holed and wasted in 2 places.","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","External Factors","","","","","wasted sections chequer plate on crossover bridge on main deck was cropped off and was fitted with inserts as required.","2023-09-15T08:00:00","","Completed","2023-08-31T08:00:00","No","No","No","Internal"]
[null,null,null,null,88166,"107_Thu Jun 01 2023 17:38:31 GMT+0800","2023-05-31T08:00:00","Defect","Ship Staff","Ship Staff Insp."," Railing on top of midship light post (port) rusted and detached.","Deck - Pipe / Fittings","Safety / LSA / FFA","Equipment Related","","","","","Replaced rusted railing with new railing. \nIssued Hot work permit and work aloft permit with office concurrence.","2023-08-30T08:00:00","","Completed","2023-08-29T08:00:00","No","No","No","Internal"]

{"sheet":"Calc","index":2,"n_rows":28,"n_cols":12,"rows_kept":28,"cut":false,"hidden":true,"merged":[]}
["Def_type","Def_cause","Equipments","VIQrefno","Observer_code"]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,"Dim itemSele As Long"]
[null,null,null,null,null,null,null,null,null,null,null,"   dim startRow as integer"]
[null,null,null,null,null,null,null,null,null,null,null,"   startRow=1"]
[null,null,null,null,null,null,null,null,null,null,null,"        For itemSele = 0 To ListBox1.ListCount - 1"]
[null,null,null,null,null,null,null,null,null,null,null,"        If ListBox1.Selected(itemSele) = True Then"]
[null,null,null,null,null,null,null,null,null,null,null,"        Worksheets(\"WorksheetName\").Range(\"A\" & startRow).Value = ListBox1.List(itemSele)"]
[null,null,null,null,null,null,null,null,null,null,null,"        startRow = startRow + 1"]
[null,null,null,null,null,null,null,null,null,null,null,"        End If"]
[null,null,null,null,null,null,null,null,null,null,null,"        Next"]
[null,null,null,null,null,null,null,null,null,null,null,"Dim LastRowA As String"]
[null,null,null,null,null,null,null,null,null,null,null,"        Dim itemSele As Long"]
[null,null,null,null,null,null,null,null,null,null,null,"       Dim startRow as integer"]
[null,null,null,null,null,null,null,null,null,null,null,"        LastRowA = ActiveSheet.Cells(Rows.count, \"A\").End(xlUp).row"]
[null,null,null,null,null,null,null,null,null,null,null,"        startQue = 0"]
[null,null,null,null,null,null,null,null,null,null,null,"        For itemSele = 0 To ListBox1.ListCount - 1"]
[null,null,null,null,null,null,null,null,null,null,null,"        For startRow = 1 To LastRowA"]
[null,null,null,null,null,null,null,null,null,null,null,"        If Worksheets(\"WorksheetName\").Range(\"A\" & startRow).Value = ListBox1.List(itemSele) Then"]
[null,null,null,null,null,null,null,null,null,null,null,"        ListBox1.Selected(itemSele) = True"]
[null,null,null,null,null,null,null,null,null,null,null,"        Exit For"]
[null,null,null,null,null,null,null,null,null,null,null,"        End If"]
[null,null,null,null,null,null,null,null,null,null,null,"        Next j"]
[null,null,null,null,null,null,null,null,null,null,null,"        Next"]
[null,null,null,null,null,null,null,null,null,null,null,"        End If"]

{"sheet":"Areaofobs","index":3,"n_rows":17,"n_cols":2,"rows_kept":17,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Cargo / Ballast Systems",11]
["Cert. & Docu.",2]
["Communication",6]
["Crew Management",3]
["Emgcy. Systems",13]
["Eng. / Strg. Comp.",14]
["General Appearance",15]
["Ice Opns.",17]
["ISM Related",7]
["ISPS Related",10]
["MARPOL Related",9]
["MLC Related",4]
["Mooring",12]
["Navigation",5]
["Safety / LSA / FFA",8]
["Structural Condn. / WT integrity ",16]

{"sheet":"Vessel_type","index":4,"n_rows":1,"n_cols":2,"rows_kept":1,"cut":false,"hidden":true,"merged":[]}
["Vessel_type","ID"]

{"sheet":"Deficiency_type","index":5,"n_rows":8,"n_cols":3,"rows_kept":8,"cut":false,"hidden":true,"merged":[]}
["TITLE","Type of deficiency_description","ID"]
["Breakdown",null,6]
["Critical Equipment",null,4]
["Defect",null,1]
["Guarantee Claim",null,8]
["Non Conformity",null,2]
["Observation",null,3]
["Other",null,7]

{"sheet":"VIQrefno","index":6,"n_rows":1,"n_cols":3,"rows_kept":1,"cut":false,"hidden":true,"merged":[]}
["VIQ_ref_no","Risk Value of observation","ID"]

{"sheet":"Equipment_list","index":7,"n_rows":28,"n_cols":3,"rows_kept":28,"cut":false,"hidden":true,"merged":[]}
["TITLE","Equipment_list_description","ID"]
["Accommodation",null,12]
["Cargo Mach.",null,13]
["Critical Equip.",null,16]
["Deck - Machinery",null,18]
["Deck - Mooring Machinery",null,15]
["Deck - Pipe / Fittings",null,20]
["Documentation",null,21]
["E/R - Air Comp.",null,8]
["E/R - Aux. Engine",null,4]
["E/R - Aux. Mach.",null,7]
["E/R - Boiler",null,5]
["E/R - Main Engine",null,3]
["E/R - Pipes/ valves & fittings",null,9]
["E/R - Pumps",null,32]
["E/R - Purifier",null,6]
["Elect. Mach. & Equip.",null,10]
["Hull & Tanks",null,19]
["Inert Gas",null,14]
["LSA / FFA",null,17]
["Miscellaneous",null,22]
["Navigation - DGPS / EPFS / AIS",null,28]
["Navigation - ECDIS",null,25]
["Navigation - Echo Sounder / Speed Log",null,26]
["Navigation - GMDSS & Communication",null,23]
["Navigation - Others",null,11]
["Navigation - RADAR",null,24]
["Navigation - VDR / BNWAS",null,30]

{"sheet":"PSC_MOU","index":8,"n_rows":11,"n_cols":3,"rows_kept":11,"cut":false,"hidden":true,"merged":[]}
["TITLE","PSC_MOU_description","ID"]
["Asia and the Pacific",null,2]
["Caribbean",null,4]
["Europe and the North Atlantic",null,1]
["Latin America",null,3]
["The Black Sea region",null,6]
["The Indian Ocean",null,8]
["The Mediterranean",null,7]
["The Riyadh MoU",null,9]
["USCG",null,10]
["West and Central Africa",null,5]

{"sheet":"Inspection_type","index":9,"n_rows":13,"n_cols":2,"rows_kept":13,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Bunkering Audit",14]
["Cargo Audit",17]
["Engineering Audit",16]
["ISM Audit",2]
["ISPS Audit",3]
["IT Audit",10]
["MLC Audit",1]
["Mooring Audit",9]
["Nav Audit / Verification",8]
["Onboard Training",18]
["Ship Staff Insp.",15]
["Suptd. Insp.",13]

{"sheet":"Deficiency_Cause","index":10,"n_rows":8,"n_cols":3,"rows_kept":8,"cut":false,"hidden":true,"merged":[]}
["TITLE","Deficiency_Cause_description","ID"]
["Behaviour Based",null,1]
["Equipment Related",null,4]
["External Factors",null,5]
["Human Error",null,7]
["Inappropriate Procedure",null,8]
["Industry Issue",null,6]
["Knowledge Based",null,3]

{"sheet":"Observer_code","index":11,"n_rows":3,"n_cols":3,"rows_kept":3,"cut":false,"hidden":true,"merged":[]}
["TITLE","Observer_code_description","ID"]
["Owner / Marine / Tech. Suptd.",null,3]
["Ship Staff",null,2]

{"sheet":"Status_code","index":12,"n_rows":6,"n_cols":3,"rows_kept":6,"cut":false,"hidden":true,"merged":[]}
["TITLE","Status_code_description","ID"]
["Completed",null,6]
["Deferred to D D",null,5]
["In progress",null,3]
["Not Started",null,2]
["Waiting spare",null,4]

{"sheet":"PSC_ref_no","index":13,"n_rows":19,"n_cols":2,"rows_kept":19,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Alarms",9]
["Cargo operations including equipment",7]
["Certificates & Documentation",2]
["Dangerous Goods",13]
["Emergency Systems",5]
["Fire safety",8]
["ISM",16]
["ISPS",17]
["Life saving appliances",12]
["MLC, 2006",18]
["Other",19]
["Pollution Prevention",15]
["Propulsion and auxiliary machinery",14]
["Radio communication",6]
["Safety of Navigation",11]
["Structural condition",3]
["Water/Weathertight condition",4]
["Working and Living Conditions",10]

{"sheet":"Risk_value_of_obs","index":14,"n_rows":1,"n_cols":2,"rows_kept":1,"cut":false,"hidden":true,"merged":[]}
["Risk Value of observation","ID"]

{"sheet":"Year","index":15,"n_rows":18,"n_cols":1,"rows_kept":18,"cut":false,"hidden":true,"merged":[]}
["Year"]
[2014]
[2015]
[2016]
[2017]
[2018]
[2019]
[2020]
[2021]
[2022]
[2023]
[2024]
[2025]
[2026]
[2027]
[2028]
[2029]
[2030]

{"sheet":"Month","index":16,"n_rows":13,"n_cols":1,"rows_kept":13,"cut":false,"hidden":true,"merged":[]}
["Month"]
["Jan"]
["Feb"]
["Mar"]
["Apr"]
["May"]
["Jun"]
["Jul"]
["Aug"]
["Sep"]
["Oct"]
["Nov"]
["Dec"]

{"sheet":"Date_","index":17,"n_rows":32,"n_cols":1,"rows_kept":32,"cut":false,"hidden":true,"merged":[]}
["Date"]
["01"]
["02"]
["03"]
["04"]
["05"]
["06"]
["07"]
["08"]
["09"]
[10]
[11]
[12]
[13]
[14]
[15]
[16]
[17]
[18]
[19]
[20]
[21]
[22]
[23]
[24]
[25]
[26]
[27]
[28]
[29]
[30]
[31]

{"sheet":"Sheet1","index":18,"n_rows":24,"n_cols":6,"rows_kept":24,"cut":false,"hidden":true,"merged":[]}
[]
[null,"ID","E",null,"Date Recorded",1]
[null,"UNIQUE ID","F",null,"Type of Deficiency",2]
[1,"Date Recorded","G",null,"Observer code",3]
["ignore","Vessel Type","H",null,"Type of Inspection",4]
[null,"Internal / External","I",null,"Description of Deficiency",5]
[null,"Drydock","J",null,"Equipment Categories",6]
[null,"Information Sharing","K",null,"Area of Observation",7]
[null,"Critical_item","L",null,"Deficiency Cause",8]
[null,"Deficiency Type","M",null,"VIQ Ref Number",9]
[null,"Deficiency Cause","N",null,"Risk Value of Obs",10]
[null,"Inspection Type","O",null,"PSC Ref Number",11]
[null,"Equipments","P",null,"PSC MOU ID",12]
[null,"VIQ Reference Number","Q",null,"Action Taken or Required",13]
[null,"Risk Value of the observation","R",null,"Target Date",14]
[null,"PSC Reference Number","S",null,"PO Ref No.",15]
[null,"PSC MOU","T",null,"Status Code",16]
[null,"Observer Code","U",null,"Date Completed",17]
[null,"Target Date","V",null,"Drydock",18]
[null,"Status Code","W",null,"Info Sharing",19]
[null,"Description of Deficiency","X",null,"Critical Item Flag",20]
[null,"Action taken / required","Y",null,"Audit Type",21]
[null,"PO ref no","Z"]
[null,"Date completed","AA"]

{"sheet":"Ship_information","index":19,"n_rows":2,"n_cols":3,"rows_kept":2,"cut":false,"hidden":true,"merged":[]}
["Ship_ID","Ship_Name","FILE_NAME"]
["107","ANTWERP (19-08-2023)","107_1693462933115.xlsm"]

{"sheet":"External_Deficiency_type","index":20,"n_rows":5,"n_cols":3,"rows_kept":5,"cut":false,"hidden":true,"merged":[]}
["TITLE","Type of deficiency_description","ID"]
["Condn of Class / Memo",null,5]
["Defect",null,1]
["Non Conformity",null,2]
["Observation",null,3]

{"sheet":"External_Inspection_type","index":21,"n_rows":11,"n_cols":2,"rows_kept":11,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Cargo Audit",17]
["Flag State Insp.",5]
["ISM Audit",2]
["ISPS Audit",3]
["MLC Audit",1]
["Nav Audit / Verification",8]
["OM Insp. (Eg. SIRE / CDI etc.)",6]
["Others (Eg. Insurance etc.)",12]
["PSC Inspection",4]
["Terminal Insp.",11]

{"sheet":"External_Observer_code","index":22,"n_rows":7,"n_cols":3,"rows_kept":7,"cut":false,"hidden":true,"merged":[]}
["TITLE","Observer_code_description","ID"]
["Class Surveyor",null,4]
["FSC Inspector",null,5]
["Others (Eg. Insurance etc.)",null,9]
["PSC Insp.",null,6]
["SIRE / CDI Insp.",null,8]
["Terminal Insp.",null,7]

{"sheet":"Sheet Version","index":23,"n_rows":2,"n_cols":2,"rows_kept":2,"cut":false,"hidden":true,"merged":[]}
["Version","Title"]
["2.0","Version 2.0"]