{"text_format":"1","workbook":"xlsx","n_sheets":24,"sheets":["Mainsheet","Completed","Calc","Areaofobs","Vessel_type","Deficiency_type","VIQrefno","Equipment_list","PSC_MOU","Inspection_type","Deficiency_Cause","Observer_code","Status_code","PSC_ref_no","Risk_value_of_obs","Year","Month","Date_","Sheet1","Ship_information","External_Deficiency_type","External_Inspection_type","External_Observer_code","Sheet Version"],"not_rendered":{"charts":0,"images":1,"macros":1,"external_links":0,"defined_names":12,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Mainsheet","index":0,"n_rows":87,"n_cols":28,"rows_kept":87,"cut":false,"hidden":false,"merged":[[10,8,10,9],[10,12,10,13],[12,6,12,27],[8,6,8,27]]}
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,"Defect - Damage Monitoring Sheet"]
[]
[null,null,null,null,null,null,null,"Date of Report","22-Oct-2023",null,null,"Ship Name","SUNRISE I (13-09-2023)"]
[]
[null,null,null,null,null,null,"VERSION : 2.0"]
[]
[]
[]
[null,null,null,"ID","SHIPSIDE UNIQUEID","UNIQUE ID","Date Recorded","Type of Deficiency","Observer code","Type of Inspection","Description of Deficiency","Equipment Categories","Area of Observation","Deficiency Cause","VIQ Ref Number","Risk Value of Obs","PSC Ref Number","PSC MOU ID","Action Taken or Required","Target Date","PO Ref No.","Status Code","Date Completed","Drydock","Info Sharing","Critical Item","Audit Type","Superintendent Remarks"]
[null,null,null,null,79013,"120_Tue Sep 27 2022 07:47:12 GMT+0800","2023-06-29T08:00:00","Defect","Ship Staff","Ship Staff Insp.","AE in and out flowmeter valves not holding same to be renewed .","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Requisition raised SUN1230130, job will be carried out as per job planning.","2023-09-29T08:00:00","SUN1230130","Waiting spare",null,"No","No","No","Internal","Already connected on board, same to renew & close out the defect in DDRL."]
[null,null,null,null,27035,"120_Sat Jul 16 2022 05:30:02 GMT+0800","2023-07-13T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Eductor Remote suction gauge in CCR was showing erratic readings.Found its Pressure transmitter malfunctioning.Steady current of 4.2 mA was measured and no change in readings while calibrating with pressure calibrator.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","Requsition raised and Spares received job will be carried out as per job planning.","2023-10-13T08:00:00","SUN1220126","Waiting spare",null,"No","No","No","Internal","Spares connected to vessel & must have been repaired. Please check & update the job accordingly."]
[null,null,null,null,15358,"0_Mon Jul 17 2023 05:02:12 GMT+0800","2023-07-15T08:00:00","Critical Equipment","Ship Staff","Ship Staff Insp.","Rotary vane steering gear top have hydraulic oil leakage","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Need to investigate and follow up with office. Vessel need shore assistance for this. Vessel need to raise RO for the same.","2023-10-06T08:00:00","","Not Started",null,"No","No","No","Internal"]
[null,null,null,null,22777,"0_Tue Jun 20 2023 21:30:33 GMT+0800","2023-07-16T08:00:00","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","1 stbd and 2 stbd bunker tank steam coils are leaking.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","1 stbd and 2 stbd bunker tank steam coil are leakings, same to be identified and necessary permanent/temporary repair work to be carried out. Leakage found to be from heater. 2Stbd heater pulled out and rectified the leak, 2Stbd heating coil is in use and under observation. Vessel need to work on 1 stbd steam coil leak.","2023-10-18T08:00:00","","In progress",null,"No","No","No","Internal"]
[null,null,null,null,86091,"120_Tue Jun 20 2023 15:57:02 GMT+0800","2023-07-16T08:00:00","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","CH no.6 and 7 hatch cover lifting jacks (fwd) observed leaking same to rectify.","Deck - Machinery","Cargo / Ballast Systems","Equipment Related","","","","","Hydraulic jack seal to be replaced. Vessel need to investigate further. Vessel require shore assistance for this job.","2023-10-18T08:00:00","","Not Started",null,"No","No","No","Internal"]
[null,null,null,null,50069,"120_Tue Jun 20 2023 20:11:10 GMT+0800","2023-07-16T08:00:00","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Cargo hold no.1 and 2 open/close hydraulic motor seal leakage to rectify.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","Hatch cover open/close hydraulic motor seal to be renewed. Need to investigate further and Vessel need to raise RO accordingly.","2023-10-18T08:00:00","","Not Started",null,"No","No","No","Internal"]
[null,null,null,null,53171,"0_Tue Jun 20 2023 22:08:34 GMT+0800","2023-07-16T08:00:00","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Rudder stock seal found to be leaking","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","Rudder stock to be greased weekly basis, with rudder movement from port to stbd. Vessel require shore assistance for this job.","2023-10-18T08:00:00","","In progress",null,"No","No","No","Internal","Vessel has received the seal to replace. Please continue greasing regularly to prevent any water leakage."]
[null,null,null,29999,47957,"120_Mon May 15 2023 00:48:43 GMT+0800","2023-07-27T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Aux Eng #1 Turbocharger Pick up Sensor is Faulty .","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Checked wiring and other connections, concluded that Pick up sensor itself is Faulty","2023-10-27T23:59:35","SUN1230070","Waiting spare",null,"No","No","No","Internal","Vessel should have spare pick up sensor on board, please check & close out DDRL."]
[null,null,null,31322,95906,"0_Thu Jun 29 2023 21:00:32 GMT+0800","2023-07-27T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Blower room scupper drains are choked.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Behaviour Based","","","","","Blower room scupper drain connecting pipes to be disconnected and cleared of debris.","2023-10-27T23:59:35","","Not Started",null,"No","No","No","Internal","Please complete this job asap."]
[null,null,null,31323,21977,"120_Thu Jun 29 2023 21:02:30 GMT+0800","2023-07-27T23:59:35","Critical Equipment","Ship Staff","Ship Staff Insp.","Aux engine lube oil storage tank outlet quick closing valve is defective. Valve no LF 17","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","New quick closing valve to be procured and replaced with defective one.","2023-10-27T23:59:35","SUN1230155","Waiting spare",null,"No","No","No","Internal","This RO has already been supplied, kindly check & close out DDRL accordingly."]
[null,null,null,null,40092,"120_Thu Jun 29 2023 21:30:38 GMT+0800","2023-07-27T08:00:00","Defect","Ship Staff","Ship Staff Insp.","7K-4K steam regulating valve is not operational. Valve no. ST05","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","New valve to be procured and replaced.","2023-10-27T08:00:00","SUN1230235","Waiting spare",null,"No","No","No","Internal","Kindly advise RO no for the valve."]
[null,null,null,null,17025,"120_Thu Jun 29 2023 22:57:24 GMT+0800","2023-07-27T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Main engine fuel oil back pressure valve is leaking/defective","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","New back pressure valve to be procured.","2023-10-27T08:00:00","SUN1230234","Waiting spare",null,"No","No","No","Internal","Kindly advise RO no for the back pressure valve."]
[null,null,null,31326,65386,"120_Thu Jun 29 2023 23:50:54 GMT+0800","2023-07-27T23:59:35","Observation","Ship Staff","Ship Staff Insp.","LSFO settling tank drain gets choked frequently.","Hull & Tanks","Eng. / Strg. Comp.","Industry Issue","","","","","LSFO settling tank bottom to be stripped and cleaned.","2023-10-27T23:59:35","","Not Started",null,"No","No","No","Internal","Kindly advise your plan to clean this LSFO settling tank."]
[null,null,null,null,16201,"120_Fri Jun 30 2023 00:29:39 GMT+0800","2023-07-27T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Fuel oil supply pump unit inbuilt inlet and outlet valves not holding. We have to stop Main engine every time we plan for filter routines.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Inlet valve, outlet valve and Non return valve to replaced with new spare. This job can only be performed during port stay.\nVALVES NOT REQUIRED, ONLY ORINGS, SAME VERIFIED AFTER OPENING AND CHECKING CONDITION OF ORINGS WHICH ARE LEAKING. NO DEFECT WITH VALVES.","2023-10-28T08:00:00","SUN1230173","Waiting spare",null,"No","No","No","Internal","Vessel has received the spares, please complete the job & update DDRL."]
[null,null,null,null,54278,"120_Fri Jun 30 2023 00:37:02 GMT+0800","2023-07-27T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Fresh water hydrophore gauge glass is defective.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","New gauge glass with sealing rings and gasket to be procured and replaced. Vessel need to raise RO.","2023-10-28T08:00:00","","Not Started",null,"No","No","No","Internal","Kindly advise RO no for our follow up."]
[null,null,null,31329,90161,"120_Mon Jul 03 2023 22:36:43 GMT+0800","2023-07-27T23:59:35","Defect","Ship Staff","Ship Staff Insp.","The Vent Flap of No 4 CH FWD STBD side , one hinge is damaged . Several other Hinges of CH Vent Flaps have thinned down.","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","Equipment Related","","","","","Require Fabrication of Hinges using Hot Work.","2023-10-27T23:59:35","","Not Started",null,"No","No","No","Internal","These job to be completed in next ballast voyage & report DDRL accordingly."]
[null,null,null,31330,75347,"120_Mon Jul 03 2023 22:41:31 GMT+0800","2023-07-27T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Several Sounding Pipes Thread Damaged for Ballast Tanks / CH  Bilges. Unable to Close Caps W/T.","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","Equipment Related","","","","","To Renew the Threads on the Male Pipe.","2023-10-28T23:59:35","","Not Started",null,"No","No","No","Internal","This is PSC matter, kindly take immediate action to repair all the sounding pipe caps."]
[null,null,null,null,58775,"120_Mon Jul 17 2023 04:33:09 GMT+0800","2023-08-15T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Main engine unit no.2 fuel pump high pressure pipe leak off line is hot a sign of oil leakage.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Fuel pump high pressure pipe to be overhauled, surfaces to be lapped for both top cover and high pressure pipes. Vessel planned to carry out this job at Vietnam.","2023-10-15T08:00:00","","Not Started",null,"No","No","No","Internal","Please complete this job at Vietnam anchorage & update DDRL."]
[null,null,null,27676,23734,"120_Tue Sep 27 2022 07:43:12 GMT+0800","2023-08-16T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Air cooler chemical cleaning tank steam coil badly corroded and wasted, has to be renewed.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","coil to be repaired/ renewed at the available opportunity","2023-10-16T23:59:35","","Deferred to D D",null,"Yes","No","No","Internal","This job spec to raise in REFMAN for next DD. Next special survey range will be July 2025.  Job to close out in DDRL once transfer to DD."]
[null,null,null,31321,69933,"120_Thu Jun 29 2023 20:58:25 GMT+0800","2023-08-27T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Oil mist box chamber scuppers are choked","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Behaviour Based","","","","","Oil mist box chamber scupper drains to be cleared, connecting pipes to be removed, and debris to be cleared.","2023-10-27T23:59:35","","Not Started",null,"No","No","No","Internal","Kindly plan this job asap & update DDRL."]
[null,null,null,null,81853,"120_Mon Sep 18 2023 15:31:16 GMT+0800","2023-09-18T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Fire and GS pump, and Fire and Bilge Pump discharge valve are leaking, not holding.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","The discharge valves for Fire and GS pump and FIre and Bilge pump are not holding. Requisition raised for the same.","2023-11-18T08:00:00","","Waiting spare",null,"No","No","No","Internal"]
[null,null,null,null,42315,"120_Tue Oct 03 2023 06:45:20 GMT+0800","2023-09-16T08:00:00","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Port and Stbd Anchor lashing eye pads found wasted to be reinforced with doubler platess","Deck - Machinery","Structural Condn. / WT integrity ","Equipment Related","","","","","","2023-10-26T08:00:00","","Not Started",null,"No","No","No","Internal"]
[null,null,null,null,63661,"0_Tue Oct 03 2023 06:47:54 GMT+0800","2023-09-16T08:00:00","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Lashing wires + Existing chains used to Lash Both Anchors to be verified ","Deck - Machinery","ISM Related","Equipment Related","","","","","","2023-10-26T08:00:00","","In progress",null,"No","No","No","Internal"]
[null,null,null,null,53402,"0_Tue Oct 03 2023 06:54:46 GMT+0800","2023-09-16T08:00:00","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Numerous ballast tank and cofferdam air vent covers metal strips are corroded and wasted. To remove and take to E/R workshop for replacement and fitted back. ","Deck - Pipe / Fittings","ISM Related","Equipment Related","","","","","","2023-10-16T08:00:00","","Not Started",null,"No","No","No","Internal"]
[null,null,null,null,18962,"0_Tue Oct 03 2023 06:57:13 GMT+0800","2023-09-16T08:00:00","Observation","Owner / Marine / Tech. Suptd.","ISM Audit","Emergency Stop box for Hatch opening has detached from frame to be welded back to position ","","ISM Related","Equipment Related","","","","","","2023-10-16T08:00:00","","Not Started",null,"No","No","No","Internal"]
[null,null,null,null,39299,"0_Tue Oct 03 2023 07:31:59 GMT+0800","2023-09-16T08:00:00","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Numerous areas on deck have material wastage ;- Railings access over pipelines + railing access to sight cargo holds +chequered plates are holed . To prepare a list of all locations with photos and invite the Engine room fitter say once or twice a week to complete the task.","Deck - Pipe / Fittings","ISM Related","Equipment Related","","","","","","2023-11-16T08:00:00","","In progress",null,"No","No","No","Internal"]
[null,null,null,null,60614,"0_Tue Oct 03 2023 07:38:36 GMT+0800","2023-09-16T08:00:00","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","FW line on deck has locations whter clamps are wasted and line is left dangling. ","Deck - Pipe / Fittings","General Appearance","Inappropriate Procedure","","","","","","2023-10-10T08:00:00","","Not Started",null,"No","No","No","Internal"]
[null,null,null,null,11114,"0_Tue Oct 03 2023 07:49:29 GMT+0800","2023-09-16T08:00:00","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","No. 6 Cargo hold fwd hydraulic piston leaking - To seek advice from Fleet 6 to replace the oil seal.","Deck - Machinery","Cargo / Ballast Systems","Equipment Related","","","","","","2023-10-15T08:00:00","","Not Started",null,"No","No","No","Internal"]
[null,null,null,null,75963,"0_Tue Oct 03 2023 07:50:29 GMT+0800","2023-09-16T08:00:00","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","No. 7 Cargo hold fwd hydraulic piston leaking - To seek advice from Fleet 6 to replace the oil seal.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","","2023-10-15T08:00:00","","Not Started",null,"No","No","No","Internal"]
[null,null,null,null,79346,"0_Tue Oct 03 2023 07:53:02 GMT+0800","2023-09-16T08:00:00","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Chequered plate Protection above on main dck stbd side i.w.o No. 6 and 7 Cargo holds - securing lig from plate to main deck is detached - same to be secured with welding.","Deck - Pipe / Fittings","ISM Related","Equipment Related","","","","","","2023-11-15T08:00:00","","Not Started",null,"No","No","No","Internal"]
[null,null,null,null,26540,"0_Tue Oct 03 2023 08:00:32 GMT+0800","2023-09-16T08:00:00","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Ballast control Room - remote pressure gauge calibration to be undertaken - no Previous record available ","E/R - Pumps","Cargo / Ballast Systems","Inappropriate Procedure","","","","","","2023-10-15T08:00:00","","Not Started",null,"No","No","No","Internal"]
[null,null,null,null,74571,"0_Tue Oct 03 2023 08:08:08 GMT+0800","2023-09-16T08:00:00","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Vessel not provided with a Compactor. ","Miscellaneous","MLC Related","Equipment Related","","","","","To check the place of installation and to order one compactor.","2023-11-15T08:00:00","","Not Started",null,"No","No","No","Internal"]
[null,null,null,null,74415,"0_Tue Oct 03 2023 08:14:11 GMT+0800","2023-09-16T08:00:00","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","O2 room rubber hose from bottle to flame arrrestor fitted with hose bands - to requisition for UNITOR approved hose and replace. ","Miscellaneous","ISM Related","Equipment Related","","","","","To order new hose and connections ","2023-11-15T08:00:00","","Not Started",null,"No","No","No","Internal"]
[null,null,null,null,94540,"120_Tue Oct 03 2023 08:39:17 GMT+0800","2023-09-16T08:00:00","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Acetylene - regulators to be replaced and must be kept within 5 years life in use.","E/R - Pipes/ valves & fittings","ISM Related","Equipment Related","","","","","","2023-11-15T08:00:00","","Not Started",null,"No","No","No","Internal"]
[null,null,null,null,78971,"0_Tue Oct 03 2023 08:41:14 GMT+0800","2023-09-16T08:00:00","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ETO workshop - spares lying on deck - shelving to be prepared , anchored to bulkhead / deck and used to stow spares ","Elect. Mach. & Equip.","General Appearance","Inappropriate Procedure","","","","","","2023-11-15T08:00:00","","Not Started",null,"No","No","No","Internal"]
[null,null,null,null,46626,"120_Tue Oct 03 2023 13:07:24 GMT+0800","2023-09-28T08:00:00","Critical Equipment","Ship Staff","Ship Staff Insp.","FIRE AND GS PUMP MECHANICAL SEAL LEAKING BADLY, VIBRATION AND UNABLE TO MAKE PRESSURE FOR EDUCTING CH BILGES","E/R - Pumps","Cargo / Ballast Systems","Equipment Related","","","","","OVERHAUL IN PROGRESS, ALL SPARES ON BOARD. OVERHAUL COMPLETED, ONLY MECHANICAL SEAL WRONG SUPPLY, AWAITING CORRECT MECHANICAL SEAL.","2023-12-13T08:00:00","SUN1230252","Waiting spare",null,"No","No","No","Internal"]
[null,null,null,null,13619,"0_Tue Oct 03 2023 13:24:44 GMT+0800","2023-09-30T08:00:00","Defect","Others (Eg. Insurance etc.)","Others (Eg. Insurance etc.)","BILGE PUMP FOR OWS HAVING REDUCED CAPACITY OF 2.2M3/HR WHEN IT SHOULD BE 5M3/HR.","Critical Equip.","MARPOL Related","Equipment Related","","","","","SUSPECT STATOR/ROTOR WORN OUT, TO REQUEST NEW SPARES","2023-12-30T08:00:00","","Not Started",null,"No","No","No","External"]
[null,null,null,null,33955,"0_Tue Oct 03 2023 16:33:01 GMT+0800","2023-09-22T08:00:00","Defect","Ship Staff","Ship Staff Insp.","#1 CH STAFFA MOTOR SEAL LEAKAGE","Cargo Mach.","Structural Condn. / WT integrity ","Equipment Related","","","","","SEALS TO RENEW","2023-12-30T08:00:00","","Not Started",null,"No","No","No","Internal"]
[null,null,null,null,26832,"0_Tue Oct 03 2023 16:34:31 GMT+0800","2023-09-26T08:00:00","Defect","Ship Staff","Ship Staff Insp.","#2 CH STAFFA MOTOR SEAL LEAKAGE","Cargo Mach.","Structural Condn. / WT integrity ","Equipment Related","","","","","TO RENEW SEAL","2023-12-30T08:00:00","","Not Started",null,"No","No","No","Internal"]
[null,null,null,null,53658,"0_Tue Oct 03 2023 16:43:14 GMT+0800","2023-09-20T08:00:00","Defect","Ship Staff","Ship Staff Insp.","SEVERAL PLUGS ON HATCH COVER JACKS LEAKING","Cargo Mach.","Structural Condn. / WT integrity ","Equipment Related","","","","","LEAKING ONES WERE RENEWED AND PLAN TO RENEW ALL SINCE MATING SURFACES ARE CORRODED.","2023-12-30T08:00:00","","In progress",null,"No","No","No","Internal"]
[null,null,null,null,64297,"0_Tue Oct 03 2023 16:53:27 GMT+0800","2023-09-27T08:00:00","Defect","Ship Staff","Ship Staff Insp.","MSW PUMP #2 MECHANICAL SEAL LEAKING","E/R - Aux. Mach.","Cargo / Ballast Systems","Equipment Related","","","","","SAME TO BE RENEWED","2023-12-30T08:00:00","","Not Started",null,"No","No","No","Internal"]
[null,null,null,null,72695,"0_Tue Oct 03 2023 16:55:46 GMT+0800","2023-09-28T08:00:00","Critical Equipment","Ship Staff","Ship Staff Insp.","BALLAST PUMP #1 LEAKAGE FROM CASING ORING, MECHANICAL SEAL LEAKAGE SUSPECTED","E/R - Pumps","Cargo / Ballast Systems","Equipment Related","","","","","SAME TO BE RENEWED AFTER OPENING FOR INSPECTION.","2023-12-30T08:00:00","","Not Started",null,"No","No","No","Internal"]
[null,null,null,null,18167,"0_Tue Oct 03 2023 17:29:17 GMT+0800","2023-09-27T08:00:00","Critical Equipment","Ship Staff","Ship Staff Insp.","INCINERATOR FLAME EYE LOCATION UNABLE TO DETECT FLAME","Critical Equip.","MARPOL Related","Equipment Related","","","","","TO ENSURE INSTALLED FLAME EYE READS THE FLAME IF PRESENT AND ENSURE NO EXTERNAL MEANS LIKE HANDLAMP ARE USED TO SIMULATE FLAME WHICH CAN HAVE DISASTROUS CONSEQUENCES","2023-12-30T08:00:00","","Not Started",null,"No","No","No","Internal"]
[null,null,null,null,91774,"0_Tue Oct 03 2023 17:31:25 GMT+0800","2023-09-21T08:00:00","Defect","Ship Staff","Ship Staff Insp.","CHAIN GUIDES WASTED IN 5 LOCATIONS AND NEED TO BE RENEWED","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","TO RENEW 5 CHAIN GUIDES","2023-12-30T08:00:00","","In progress",null,"No","No","No","Internal"]
[null,null,null,null,22245,"0_Tue Oct 03 2023 19:27:19 GMT+0800","2023-09-30T08:00:00","Defect","Ship Staff","Ship Staff Insp.","AE 1 TURBOCHARGER RPM PICKUP NOT FUCTIONAL","Critical Equip.","Emgcy. Systems","Equipment Related","","","","","WRONG SUPPLY, TO SUPPLY CORRECT SPARE AS PER SPECS SENT IN REQUISITION","2023-12-30T08:00:00","","Not Started",null,"No","No","No","Internal"]
[null,null,null,null,88130,"0_Tue Oct 03 2023 19:29:30 GMT+0800","2023-10-01T08:00:00","Critical Equipment","Ship Staff","Ship Staff Insp.","ALARM DISPLAY PANEL NOT WORKING, SAME REQUESTED FOR ADVICE OR SPARE","Critical Equip.","Emgcy. Systems","Equipment Related","","","","","Troubleshooting was carried out and we tried changing its VGA cable and connected it to another monitor and same message was shown in monitor.\nSystem processing unit was opened, Hard drive , RAM and DSN PCI PC card, cooling fan were inspected.\nFollowing observations were made,\n1.\tThere is no noise/sound in hard drive while system is starting.\n2.\tCooling fan is running.\n3.\tProcessor LED’s are lit.\n4.\tDSN PCI PC card All Status LED’s are not lit as shown in attached picture.\n5.\tNo burnt mark, abnormality was seen in processing unit.\n","2023-12-30T08:00:00","","Waiting spare",null,"No","No","No","Internal"]
[null,null,null,null,44275,"0_Tue Oct 03 2023 19:31:06 GMT+0800","2023-09-17T08:00:00","Critical Equipment","Ship Staff","Ship Staff Insp.","ACCUMULATOR OF R/BOAT DAVIT HYDRAULIC UNIT LEAKING AND OUT OF OPERATION","Critical Equip.","Emgcy. Systems","Equipment Related","","","","","TO RENEW SINCE INTERNAL LEAK","2023-12-30T08:00:00","","Not Started",null,"No","No","No","Internal"]
[null,null,null,null,80847,"0_Tue Oct 03 2023 19:32:34 GMT+0800","2023-09-30T08:00:00","Defect","Ship Staff","Ship Staff Insp.","ALFA LUBRICATOR ACCUMULATOR LEAK","Critical Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","TO RENEW WITH SPARE ALREADY RECEIVED WHEN M/E IN STOP CONDITION","2023-12-30T08:00:00","SUN1230224  ALPHA LUBRICATOR - SPARES ","In progress",null,"No","No","No","Internal"]
[null,null,null,null,58540,"0_Tue Oct 03 2023 19:38:00 GMT+0800","2023-10-03T08:00:00","Defect","Ship Staff","Ship Staff Insp.","PRIMING UNITS OF FIRE AND GS PUMP, FIRE AND BILGE PUMP AND OTHER CENTRIFUGAL PUMPS NOT OPERATIONAL AND NOT TRIED OUT","E/R - Pumps","Cargo / Ballast Systems","Equipment Related","","","","","TO RECTIFY AND TRY OUT REGULARLY TO ENSURE CORRECT WORKING","2023-12-30T08:00:00","","In progress",null,"No","No","No","Internal"]
[null,null,null,null,67193,"0_Tue Oct 03 2023 19:39:54 GMT+0800","2023-10-03T08:00:00","Defect","Ship Staff","Ship Staff Insp.","SEVERAL VALVES IN ENGINEROOM NOT HOLDING AND A FEW FOUND FROZEN DUE TO NOT IN REGULAR USE.","E/R - Pipes/ valves & fittings","Cargo / Ballast Systems","Equipment Related","","","","","SAME TO BE EASED UP AND TRIED OUT REGULARLY","2023-12-30T08:00:00","","In progress",null,"No","No","No","Internal"]
[null,null,null,null,31932,"0_Tue Oct 03 2023 19:43:53 GMT+0800","2023-10-03T08:00:00","Critical Equipment","Ship Staff","Ship Staff Insp.","RUDDER STOCK LUBE OIL LEAK FROM ORING","Critical Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","SAME TO BE RENEWED AND LEAK ARRESTED","2023-12-30T08:00:00","","Not Started",null,"No","No","No","Internal"]
[null,null,null,null,21694,"0_Tue Oct 03 2023 19:45:27 GMT+0800","2023-10-01T08:00:00","Defect","Ship Staff","Ship Staff Insp.","STERN TUBE FWD SEAL LEAKAGE","Critical Equip.","Emgcy. Systems","Equipment Related","","","","","TO RENEW THE SEAL AND ARREST LEAKAGE","2023-12-30T08:00:00","","Deferred to D D",null,"No","No","No","Internal"]
[null,null,null,null,35720,"120_Fri Oct 06 2023 12:56:50 GMT+0800","2023-09-10T08:00:00","Critical Equipment","Ship Staff","Ship Staff Insp.","AE 2 STATOR WINDING T SENSOR FAIL ALARM ","Critical Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","TO RENEW SENSOR, RECTIFY ISSUE","2023-12-30T08:00:00","","Not Started",null,"No","No","No","Internal"]
[null,null,null,null,44263,"0_Fri Oct 06 2023 13:04:09 GMT+0800","2023-09-14T08:00:00","Critical Equipment","Ship Staff","Ship Staff Insp.","FUEL MODULE SUPPLY PUMP SUCTION DISCHARGE VALVES NOT HOLDING, AND VESSEL FOLLOWING A PROCEDURE OF CHANGING OVER AUX ENGINES TO LSMGO AND STOPPING M/E  AND MODULE TO ENABLE FILTER CLEANING. THIS IS RISKY IN BAD  WEATHER/ PILOTAGE/NARROW WATERS IF FILTERS GET FOULED WITH BAD BUNKERS AND MAIN ENGINE HAS TO BE STOPPED TO CLEAN FILTERS. VERY RISKY WITH BAD BUNKER WHERE FREQUENT FILTER CLEANING IS REQUIRED AND MAIN ENGINE CANNOT BE STOPPED FREQUENTLY WITH THIS SERIOUS OPERATIONAL LAPSE.","Critical Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","TO REQUEST NEW VALVES AND FIT SINCE THIS IS VERY RISKY OPERATION IF NO OPPORTUNITY TO STOP MAIN ENGINE.","2023-12-31T08:00:00","","Not Started",null,"No","No","No","Internal"]
[null,null,null,null,10094,"0_Mon Oct 09 2023 12:22:37 GMT+0800","2023-10-01T08:00:00","Defect","Ship Staff","Ship Staff Insp.","OWS BILGE PUMP FOUND PUMPING ONLY 2.2 M3/HR WHEN CAPACITY IS 5 M3/HR","Critical Equip.","MARPOL Related","Equipment Related","","","","","TO RENEW STATOR/ROTOR AS REQUIRED TO ATTAIN DESIGN CAPACITY TO AVOID RUNNING OWS LONGER TIME.","2023-12-30T08:00:00","","Waiting spare",null,"No","No","No","Internal"]
[null,null,null,null,31557,"0_Tue Oct 10 2023 10:29:04 GMT+0800","2023-09-27T08:00:00","Critical Equipment","Ship Staff","Ship Staff Insp.","TRO REPEATED ALARMS","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","TO CHECK QUALITY AND EXPIRY DATE OF CHEMICALS IN USE AND RENEW IF REQUIRED","2023-12-26T08:00:00","","In progress",null,"No","No","No","Internal"]
[null,null,null,null,23641,"120_Tue Oct 10 2023 11:06:19 GMT+0800","2023-09-24T08:00:00","Defect","Ship Staff","Ship Staff Insp.","REEFER #2 CONDENSER OUTLET VALVE LEAKING.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","TO REQUEST VALVE AND RENEW","2023-12-23T08:00:00","","Not Started",null,"No","No","No","Internal"]
[null,null,null,null,34674,"0_Tue Oct 10 2023 11:08:23 GMT+0800","2023-09-28T08:00:00","Defect","Ship Staff","Ship Staff Insp.","AIRCON VALVES BEFORE AND AFTER DRYER NOT HOLDING, DRYER NOT RENEWED FOR LONG TIME.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","TO RENEW VALVES AND/OR ARREST LEAKAGE FROM VALVES","2023-12-27T08:00:00","","Not Started",null,"No","No","No","Internal"]
[null,null,null,null,20965,"120_Sat Oct 14 2023 11:41:22 GMT+0800","2023-09-29T08:00:00","Critical Equipment","Ship Staff","Ship Staff Insp.","PROV CRANE LUFFING MOTOR MAGNETIC BRAKE DEFECTIVE AND DRAWING MORE CURRENT. ","Critical Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","CHECKED HOISTING AND SLEWING BRAKE CLEARANCE, RENEWED ALL 7 LIMIT SWITCHES. PENDING SUPPLY FOR MAGNETIC BRAKE FOR LUFFING MOTOR.","2023-12-01T08:00:00","SUN1230247 PROVISION CRANE","Waiting spare",null,"No","No","No","Internal"]
[null,null,null,null,15716,"120_Sat Oct 14 2023 11:47:01 GMT+0800","2023-09-29T08:00:00","Critical Equipment","Ship Staff","Ship Staff Insp.","FUEL OIL SUPPLY SYSTEM LOCAL PANEL PUSH BUTTONS FOR STARTING PUMPS DEFECTIVE, LOCAL OPERATION NOT POSSIBLE","Critical Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","TO RENEW PUSH BUTTONS AFTER RECEIVING SPARES","2023-12-01T08:00:00","SUN1230237 FUEL OIL SUPPLY SYSTEMS","Waiting spare",null,"No","No","No","Internal"]
[null,null,null,null,41283,"120_Sat Oct 14 2023 11:51:26 GMT+0800","2023-09-28T08:00:00","Critical Equipment","Ship Staff","Ship Staff Insp.","AUX ENGINE HEATER FOR FO SUPPLY SYSTEMS THERMOSTAT DEFECTIVE","E/R - Aux. Engine","Emgcy. Systems","","","","","","TO MAKE OPERATIONAL ON SUPPLY OF SPARES","2024-01-31T08:00:00","SUN1230237 FUEL OIL SUPPLY SYSTEMS","Waiting spare",null,"No","No","No","Internal"]
[null,null,null,null,54260,"120_Thu Oct 19 2023 09:34:16 GMT+0800","2023-10-11T08:00:00","Defect","Ship Staff","Ship Staff Insp.","CARGO HOLD NO.7 FWD ACCESS HATCH HINGE BROKEN FROM FOUNDATION. ","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","Equipment Related","","","","","REQUIRED TO FABRICATE NEW HINGE AND WELD TO FOUNDATION ","2023-11-11T08:00:00","","Not Started",null,"No","No","No","Internal"]
[null,null,null,null,84331,"120_Thu Oct 19 2023 13:34:24 GMT+0800","2023-10-19T08:00:00","Defect","Ship Staff","Ship Staff Insp.","STBD WIPER OF BRIDGE FWD WIND SHIELDS NOT OPERATIONAL","Navigation - Others","Navigation","Equipment Related","","","","","TO RECTIFY AND REQUEST THE PARTS IF NOT ALREADY ","2023-11-19T08:00:00","","In progress",null,"No","No","No","Internal"]
[null,null,null,null,61459,"120_Sun Oct 22 2023 11:25:13 GMT+0800","2023-09-29T08:00:00","Critical Equipment","Ship Staff","Ship Staff Insp.","THREE LIMITS NOT WORKING EVEN AFTER LIMIT SWITCH RENEWAL.","Deck - Machinery","Eng. / Strg. Comp.","Equipment Related","","","","","TROUBLE SHOOTING IN PROGRESS","2023-12-15T08:00:00","","In progress",null,"No","No","No","Internal"]
[null,null,null,null,67543,"0_Sun Oct 22 2023 11:29:52 GMT+0800","2023-09-29T08:00:00","Breakdown","Ship Staff","Ship Staff Insp.","MEAT ROOM DOOR HEATER NOT OPERATIONAL","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","TO RENEW","2023-12-15T08:00:00","","Not Started",null,"No","No","No","Internal"]
[null,null,null,null,32682,"0_Sun Oct 22 2023 11:31:12 GMT+0800","2023-09-28T08:00:00","Critical Equipment","Ship Staff","Ship Staff Insp.","R/BOAT AND L/BOAT COMPASS LIGHT DEFECTIVE","Critical Equip.","Emgcy. Systems","Equipment Related","","","","","TO RENEW","2023-12-13T08:00:00","","Waiting spare",null,"No","No","No","Internal"]
[null,null,null,null,15247,"0_Sun Oct 22 2023 11:32:40 GMT+0800","2023-09-27T08:00:00","Critical Equipment","Ship Staff","Ship Staff Insp.","FUEL TANKS GAUGES INACCURATE","Critical Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","TO CALIBERATE OR RENEW","2023-12-19T08:00:00","","In progress",null,"No","No","No","Internal"]
[null,null,null,null,80445,"0_Sun Oct 22 2023 11:34:07 GMT+0800","2023-09-17T08:00:00","Critical Equipment","Ship Staff","Ship Staff Insp.","#5 CARGO HOLD WATER INGRESS ALARM DEFECTIVE","Critical Equip.","Cargo / Ballast Systems","Equipment Related","","","","","CHECKED AND FOUND NEEDS RENEWAL. ","2023-12-15T08:00:00","","In progress",null,"No","No","No","Internal"]
[null,null,null,null,86087,"0_Sun Oct 22 2023 11:49:09 GMT+0800","2023-09-28T08:00:00","Critical Equipment","Ship Staff","Ship Staff Insp.","3 GREEN NAVIGATION LIGHTS FOR SINGAPORE TRANSIT FOUNDATION PLATE WASTED","Critical Equip.","Navigation","Equipment Related","","","","","TO RENEW AND REFIT LIGHTS","2023-12-27T08:00:00","","Not Started",null,"No","No","No","Internal"]
[null,null,null,null,18986,"0_Sun Oct 22 2023 11:50:35 GMT+0800","2023-09-25T08:00:00","Critical Equipment","Ship Staff","Ship Staff Insp.","FWD WHISTLE FOUNDATION BOLTS WASTED","Critical Equip.","Navigation","Equipment Related","","","","","SAME TO RENEW AND SECURE","2023-12-27T08:00:00","","Not Started",null,"No","No","No","Internal"]

{"sheet":"Completed","index":1,"n_rows":167,"n_cols":28,"rows_kept":167,"cut":false,"hidden":false,"merged":[[10,8,10,9],[10,12,10,13],[12,6,12,27],[8,6,8,27]]}
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,"Defect - Damage Monitoring Sheet"]
[]
[null,null,null,null,null,null,null,"Date of Report","22-Oct-2023",null,null,"Ship Name","SUNRISE I (13-09-2023)"]
[]
[null,null,null,null,null,null,"VERSION : 2.0"]
[]
[]
[]
[null,null,null,"ID","SHIPSIDE UNIQUEID","UNIQUE ID","Date Recorded","Type of Deficiency","Observer code","Type of Inspection","Description of Deficiency","Equipment Categories","Area of Observation","Deficiency Cause","VIQ Ref Number","Risk Value of Obs","PSC Ref Number","PSC MOU ID","Action Taken or Required","Target Date","PO Ref No.","Status Code","Date Completed","Drydock","Info Sharing","Critical Item","Audit Type","Superintendent Remarks"]
[null,null,null,21794,null,"120_10/23/2021 10:36:10 AM","2021-06-02T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Auxilliary Engine turbocharger rpm not indicating on monitor display.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Speed sensor replaced.","2021-07-03T23:59:35","","Completed","2021-10-19T23:59:35","No","No","No","Internal"]
[null,null,null,20465,null,"120_7/25/2021 5:45:38 PM","2021-06-29T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Ship Staff Insp.","THE F.O. FILTER AUTO BACKWASH IS STUCK UP","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","REPAIRED BY ELECTRICIAN","2021-09-12T23:59:35","NO REQ. YET","Completed","2021-05-01T23:59:35","No","No","No","Internal"]
[null,null,null,21080,null,"120_8/27/2021 12:28:29 PM","2021-07-05T23:59:35","Critical Equipment","Owner / Marine / Tech. Suptd.","Engineering Audit","G/E#3 Cylinder cover #3&4 leaking","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","RE-TIGHTENED BY HYDRAULIC JACK","2021-08-23T23:59:35","FANT210008 D/G SPARES","Completed","2021-08-08T23:59:35","No","No","No","Internal"]
[null,null,null,21081,null,"120_8/27/2021 2:55:40 PM","2021-07-08T23:59:35","Breakdown","Owner / Marine / Tech. Suptd.","Engineering Audit","M/E RPM indicator defective","Critical Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","REPPAIRED BY ELECTRICIAN","2021-08-23T23:59:35","","Completed","2021-08-15T23:59:35","No","No","No","Internal"]
[null,null,null,21082,null,"120_8/27/2021 3:01:12 PM","2021-07-11T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Engineering Audit","Galley griller low insulation","Elect. Mach. & Equip.","Safety / LSA / FFA","Equipment Related","","","","","REPAIRED BY ELECTRICIAN","2021-08-23T23:59:35","","Completed","2021-11-30T23:59:35","No","No","No","Internal"]
[null,null,null,20466,null,"120_7/25/2021 11:00:13 PM","2021-07-17T23:59:35","Defect","Ship Staff","Ship Staff Insp.","FIRE FIGHTING UHF RADIOS NOT WORKING/ DEFECTIVE","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","RECEIVED NEW FIRE FIGHTING UHF RADIOS AND REPLACED DEFECTIVE RADIOS","2021-04-01T23:59:35","SUN1210046","Completed","2021-04-01T23:59:35","No","No","No","Internal","UHF radios are in order & will be connected at next convenient port."]
[null,null,null,21077,null,"120_17-08-21 10:36:23 AM","2021-07-20T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Gas sampling point CH no.7 p+s & CH no.6 p/s not properly closing due to rust & deterioration.","Deck - Pipe / Fittings","General Appearance","External Factors","","","","","repaired ","2021-08-04T23:59:35","","Completed","2021-08-04T23:59:35","No","No","No","Internal"]
[null,null,null,20468,null,"120_8/2/2021 1:18:42 PM","2021-07-22T23:59:35","Defect","Ship Staff","Ship Staff Insp.","damaged pilot ladder drum reel bearing housing and chain coupling","Deck - Machinery","General Appearance","External Factors","","","","","Repaired pilot ladder drum reel bearing housing and chain coupling after received spares. tested and working in normal condition","2021-08-21T23:59:35","SUN1210049","Completed","2021-08-21T23:59:35","No","No","No","Internal","Spares are in order, will be connected vessel at convenient port."]
[null,null,null,21795,null,"120_22/10/2021 18:37:42","2021-09-02T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Main cooling sea water pump #2 overload trip","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Replaced motor bearing ,found working satisfactorily.","2021-10-03T23:59:35","","Completed","2021-10-14T23:59:35","No","No","No","Internal"]
[null,null,null,21790,null,"120_22/10/2021 19:20:43","2021-09-10T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Fish room in Galley found unable to maintain -16° temperature","Accommodation","MLC Related","Equipment Related","","","","","Need to be checked by ETO & repair if necessary.","2021-10-22T23:59:35","","Completed","2021-09-30T23:59:35","No","No","No","Internal"]
[null,null,null,21788,null,"120_10/25/2021 8:50:05 AM","2021-09-15T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Fire & GS pump not operational","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","","","","","Motor bearing renewed.tried out pump found working satisfctorily.","2021-11-15T23:59:35","","Completed","2021-10-19T23:59:35","No","No","No","Internal"]
[null,null,null,21792,null,"120_24/10/2021 10:56:05","2021-09-17T23:59:35","Non Conformity","Ship Staff","Ship Staff Insp.","Port side Pilot Ladder, bottom two steps found deformed, embarkation ladder for liferaft found in poor shape. ","LSA / FFA","Safety / LSA / FFA","Knowledge Based","","","","","PO raised, awaiting berthing of vessel.","2021-11-07T23:59:35","SUN1210108 - PILOT AND EMBARKATION LADDER","Completed","2021-10-19T23:59:35","No","No","No","Internal"]
[null,null,null,21793,null,"120_24/10/2021 12:08:42","2021-09-17T23:59:35","Defect","Ship Staff","Ship Staff Insp.","VRCS accumulator found empty, due to which hydraulic pump for VRCS was running contniously","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","Check availability of nitrogen and top up accummulators on main deck.","2021-10-01T23:59:35","","Completed","2021-09-27T23:59:35","No","No","No","Internal"]
[null,null,null,21796,null,"120_10/25/2021 8:59:10 AM","2021-10-03T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Start motor not available for aux. engine","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Start air motor recieved and installed.","2022-08-25T23:59:35","","Completed","2022-03-11T23:59:35","No","No","No","Internal"]
[null,null,null,21797,null,"120_24/10/2021 12:12:41","2021-10-03T23:59:35","Non Conformity","Ship Staff","Ship Staff Insp.","Forcastle water tight door and cargo hold booby hatch cover's found not closing / opening properly.","Hull & Tanks","Structural Condn. / WT integrity ","External Factors","","","","","Derusting/ Renewal of gasket and greasing of all nipples to be carried out.","2021-11-22T23:59:35","","Completed","2021-10-26T23:59:35","No","No","No","Internal","Please try to get this job completed at this anchorage."]
[null,null,null,26983,null,"120_Mon Sep 26 2022 01:58:45 GMT+0000","2021-10-04T23:59:35","Observation","PSC Insp.","PSC Inspection","The rating of appropriate setting of the overload protective device for each circuit shall be permanently  indicated at the location of the protective device. PSCO observed 03 unlabeled breakers, 2 on main switchboard and 1 on emergency switchboard","","General Appearance","","","","Other","","","2021-10-18T23:59:35","","Completed","2021-10-11T23:59:35","No","No","No","External"]
[null,null,null,21799,null,"120_10/22/2021 10:37:55 PM","2021-10-14T23:59:35","Critical Equipment","Ship Staff","Nav Audit / Verification","Ship's whistle air line on Monkey Island leaking air.","Navigation - Others","Navigation","External Factors","","","","","Need to replace new air pipe","2021-11-03T23:59:35","","Completed","2021-10-18T23:59:35","No","No","No","Internal"]
[null,null,null,21800,null,"120_22/10/2021 18:48:37","2021-10-14T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Air line on midship found holed, due to corrosion","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","External Factors","","","","","Need renewal of air line flange to flange.","2021-11-14T23:59:35","","Completed","2021-10-17T23:59:35","No","No","No","Internal"]
[null,null,null,21801,null,"120_22/10/2021 19:16:34","2021-10-14T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Steering compartment boiler platform door found to be lashed with wire in open condition","Miscellaneous","Crew Management","Behaviour Based","","","","","Need to check all doors in Engine room and remove all temporary arrangement made to keep door open all times.","2021-10-17T23:59:35","","Completed","2021-10-16T23:59:35","No","No","No","Internal"]
[null,null,null,20469,null,"120_8/9/2021 9:50:30 AM","2021-10-31T23:59:35","Observation","Ship Staff","Ship Staff Insp.","letters and numbers on the auto pilot information display sometimes changes and become other number, letter or character","Navigation - Others","General Appearance","Equipment Related","","","","","requested guidance, system reboot carried out.","2022-11-22T23:59:35","","Completed","2023-01-11T23:59:35","No","No","No","Internal","Arranged technician to attend vessel at Fujairah. Please close out if rectified."]
[null,null,null,21804,null,"120_10/25/2021 8:55:06 AM","2021-11-08T23:59:35","Defect","Ship Staff","Ship Staff Insp.","MEFO Auto back was filter is not working","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Limit switch replaced , found working satisfactory.","2022-02-07T23:59:35","","Completed","2021-12-23T23:59:35","No","No","No","Internal"]
[null,null,null,20467,null,"120_7/25/2021 5:19:21 PM","2021-11-10T23:59:35","Defect","Ship Staff","Ship Staff Insp.","HIGH TEMP. ALARM ON THE CONTROL AIR DRIER","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","PRESENTLY NO ALARM","2022-02-09T23:59:35","NO REQ. YET","Completed","2022-03-11T23:59:35","No","No","No","Internal"]
[null,null,null,21789,null,"120_10/25/2021 9:23:56 AM","2021-11-11T23:59:35","Critical Equipment","Ship Staff","Ship Staff Insp.","Incinerator Opeartion firing in LSMGO but after 25 min after activation of secondary burner , the secondary chamber no reaching to the  temperature of 650deg","Critical Equip.","MARPOL Related","Equipment Related","","","","","Burner nozzle changed and electrodes changed., after receiving spares in Singapore. tried out ,now temperature reaching above 650 deg . in secondary chamber.\n","2022-08-23T23:59:35","","Completed","2022-08-10T23:59:35","No","No","No","Internal","Follow up with maker & vessel being done, incinerator made operation but at full capacity. Further checks & follow up being done."]
[null,null,null,20461,null,"120_7/25/2021 5:35:09 PM","2021-11-12T23:59:35","Defect","Ship Staff","Ship Staff Insp.","DEIFECTIVE PLC AND SOLENOID VALVE OF THE PACK AIRCON IN ECR.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","CIRCUIT HAS BEEN CHANGED FOUND OPERATIONAL.","2022-02-12T23:59:35","NO REQ. YET","Completed","2022-01-18T23:59:35","No","No","No","Internal","Vessel to follow up with Auto Electrical support for trouble shooting & thereafter to raise raise RO if require any."]
[null,null,null,21798,null,"120_22/10/2021 15:03:27","2021-11-14T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Pressure gauges in Engine room machinary found opaque, unable to read through them.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Industry Issue","","","","","Identified and renewed pressure gauges as required.","2022-05-22T23:59:35","","Completed","2022-05-17T23:59:35","No","No","No","Internal","Waiting for RO to arrange supply."]
[null,null,null,21802,null,"120_22/10/2021 19:26:19","2021-11-14T23:59:35","Observation","Ship Staff","Ship Staff Insp.","MSMP manual found equipment code is wrong, due to which MBL & BHC calculated is wrong. Need to correct on Manual and mooring winches.","Deck - Mooring Machinery","Mooring","Knowledge Based","","","","","MSMP  manual updated with correct equipment code  and  all mooring winches corrected for BHC.","2022-02-13T23:59:35","","Completed","2022-03-29T23:59:35","No","No","No","Internal","Please check & correct asap."]
[null,null,null,21791,null,"120_10/25/2021 9:07:14 AM","2021-11-15T23:59:35","Observation","Ship Staff","Ship Staff Insp.","No sludge evaporation from incinerator waste oil service tank.","Hull & Tanks","MARPOL Related","Equipment Related","","","","","tank already cleaned , steam trap and coil  checked , evaporation rate has improved ","2022-10-23T23:59:35","","Completed","2022-08-24T23:59:35","No","No","No","Internal","Waste oil tank heating coil & tank to clean, return line steam trap to check / overhaul as necessary."]
[null,null,null,20463,null,"120_7/25/2021 5:27:08 PM","2021-11-20T23:59:35","Defect","Ship Staff","Ship Staff Insp.","MOTOR AND FAN OVERLOAD ALARM OF DECK AIR COMPRESSOR","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","Maker attendedance,checked PLC controller, modify phase sequence relay K25 and made compresor operational","2022-02-19T23:59:35","SPARE RECIEVED ON BOARD","Completed","2021-12-22T23:59:35","No","No","No","Internal"]
[null,null,null,20464,null,"120_7/25/2021 5:41:07 PM","2021-11-21T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Ship Staff Insp.","THE FLOWMETER READING IS NOT ACCURATE","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","the total flowmeter reading is working but the AE in and out is not functioning, same to be checked. Requisition raised. duplicate defect job order.","2023-01-23T23:59:35","","Completed","2023-01-11T23:59:35","No","No","No","Internal","Vessel to follow up with office on flowmeter issue."]
[null,null,null,23576,null,"120_15/11/2021 11:10:13","2021-11-22T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Found water ingress in # 4 Lower Stool and Lower Stool suction valve un-operational.","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","Equipment Related,External Factors","","","","","All valves over hauled and DB tanks manholes power tooled and painted. Further verified and found no more ingress of water in any stool space.","2022-07-25T23:59:35","","Completed","2022-02-07T23:59:35","No","No","No","Internal"]
[null,null,null,20462,null,"120_7/25/2021 5:14:16 PM","2021-11-22T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Ship Staff Insp.","DEFECTIVE CPU OF THE NO. 2  AMS IN ECR","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","WORKIG SATISFACTORILY.","2022-02-20T23:59:35","SUN1210045","Completed","2022-05-29T23:59:35","No","No","No","Internal","New one will be connected at next convenient port."]
[null,null,null,21803,null,"120_10/25/2021 8:38:58 AM","2021-12-03T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Deck compressor not operational, to be investigated","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related","","","","","Maker attended,checked PLC controller, modify phase sequence relay K25 and made compressor operational.","2022-08-25T23:59:35","","Completed","2021-12-22T23:59:35","No","No","No","Internal"]
[null,null,null,24640,null,"120_3/22/2022 8:55:42 PM","2022-03-09T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","incinerator primary burner firing erratically","Critical Equip.","Eng. / Strg. Comp.","Equipment Related","","","",""," Job double up .Troubleshooting  is in progress. ","2022-06-22T23:59:35","","Completed","2022-06-02T23:59:35","No","No","No","Internal"]
[null,null,null,24642,null,"120_3/22/2022 9:13:05 PM","2022-03-09T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","engine room save all trays to clean paint after leakages rectification.","Miscellaneous","General Appearance","Equipment Related","","","","","engine room save all trays cleaned painted after leakages rectification. ","2022-04-14T23:59:35","","Completed","2022-04-07T23:59:35","No","No","No","Internal"]
[null,null,null,24643,null,"120_3/22/2022 9:15:53 PM","2022-03-09T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","faulty level gauge of fresh water tank.","Hull & Tanks","Eng. / Strg. Comp.","Equipment Related","","","","","level Gauge renewed with spare one received in Singapore","2022-08-23T23:59:35","SUN 1220048","Completed","2022-08-14T23:59:35","No","No","No","Internal"]
[null,null,null,24644,null,"120_3/22/2022 9:18:28 PM","2022-03-09T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","fresh water generator out of service","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","Fresh water generator put into service ,all parameters checked found satisfactory","2022-08-23T23:59:35","","Completed","2022-07-02T23:59:35","No","No","No","Internal"]
[null,null,null,24645,null,"120_3/22/2022 9:26:11 PM","2022-03-09T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","boiler sampling cock and various valves found wrapped with tape to stop leakges from gasket","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","identification and rectification of leakages is done. ","2022-04-22T23:59:35","","Completed","2022-04-18T23:59:35","No","No","No","Internal"]
[null,null,null,24646,null,"120_3/22/2022 9:30:05 PM","2022-03-09T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ballast valve BA 102 not holding, seat ring to renew","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","BA 102 ballast valve seat ring found in good condition, assembled back the same.and changed complete valve with seat ring for BA 101","2022-06-08T23:59:35","","Completed","2022-05-27T23:59:35","No","No","No","Internal"]
[null,null,null,24647,null,"120_3/22/2022 9:33:46 PM","2022-03-09T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","permanent repair by welding insert to be carried out for ballast line ( inlet to ballast pump no.1 ) with temporary repair","E/R - Pipes/ valves & fittings","Structural Condn. / WT integrity ","Equipment Related","","","","","Permanent repair made with welding insert.","2022-06-08T23:59:35","","Completed","2022-08-27T23:59:35","No","No","No","Internal"]
[null,null,null,24648,null,"120_3/22/2022 9:45:18 PM","2022-03-09T23:59:35","Observation","Others (Eg. Insurance etc.)","Suptd. Insp.","several gauges broken, same to rectify","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","identify faulty gauges and replaced with new one.","2022-05-23T23:59:35","","Completed","2022-05-17T23:59:35","No","No","No","Internal"]
[null,null,null,24649,null,"120_3/22/2022 9:48:23 PM","2022-03-09T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","several leakages observed on all 3 auxiliary engines, leakaes to be rectify.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","identified and leakage rectification is done .","2022-04-22T23:59:35","","Completed","2022-04-18T23:59:35","No","No","No","Internal"]
[null,null,null,24650,null,"120_3/22/2022 9:54:45 PM","2022-03-09T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","engine room tank top and bilge well found oil traces, same to clean and paint","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","Engine room tank top cleaned and painted. ","2022-04-22T23:59:35","","Completed","2022-04-22T23:59:35","No","No","No","Internal"]
[null,null,null,24652,null,"120_3/22/2022 10:01:13 PM","2022-03-09T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","various pumps leakages in purifier room to be rectified. ","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","","","","","identification of leakges  carried out and rectified the same.","2022-04-22T23:59:35","","Completed","2022-04-06T23:59:35","No","No","No","Internal"]
[null,null,null,24656,null,"120_3/22/2022 9:50:56 PM","2022-03-09T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","all 3 generators insulation cladding is damaged, same to rectify. ","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","insulation cladding replaced for all generators","2022-04-22T23:59:35","","Completed","2022-04-22T23:59:35","No","No","No","Internal"]
[null,null,null,24657,null,"120_3/22/2022 8:38:53 PM","2022-03-09T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","no.2 lub oil purifier op board faulty","E/R - Purifier","Eng. / Strg. Comp.","Equipment Related","","","",""," Faulty op board changed with new one.","2022-03-27T23:59:35","","Completed","2022-03-15T23:59:35","No","No","No","Internal"]
[null,null,null,24658,null,"120_3/22/2022 9:01:07 PM","2022-03-09T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","forward ICCP faulty","Hull & Tanks","Structural Condn. / WT integrity ","Equipment Related","","","","","cofferdam cleanedand made dry, renewed cable found working satisfactorily.","2022-06-08T23:59:35","","Completed","2022-03-11T23:59:35","No","No","No","Internal"]
[null,null,null,24659,null,"120_3/22/2022 9:36:16 PM","2022-03-09T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","hfo service/settling tank cleaning to be carried out. ","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","hfo service and settling tank cleaning completed.","2022-03-27T23:59:35","","Completed","2022-03-17T23:59:35","No","No","No","Internal"]
[null,null,null,24660,null,"120_3/22/2022 9:22:53 PM","2022-03-09T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","LT cooler various valves gaskets leakages to be rectified.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","Leakages was taking place from sacrificial flanges, same renewed and rectified leak.","2022-03-16T23:59:35","","Completed","2022-03-18T23:59:35","No","No","No","Internal"]
[null,null,null,24661,null,"120_3/22/2022 8:28:03 PM","2022-03-09T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","sewage treatment plant low level alarm malfuctioning due to which pump keeps running continuously and do not stop.","Miscellaneous","MARPOL Related","Equipment Related","","","","","High level switch renewed,low level swich rectified,Circuit modification removed. ","2022-03-27T23:59:35","","Completed","2022-03-11T23:59:35","No","No","No","Internal"]
[null,null,null,24662,null,"120_22/03/2022 12:00:38","2022-03-09T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Engineering Audit","Alarm monitoring system repater panel on bridge all LED lights are lit up","Elect. Mach. & Equip.,Navigation - Others","Communication","Equipment Related","","","","","Pressed S3 button on panel, issue resolved","2022-04-09T23:59:35","","Completed","2022-03-11T23:59:35","No","No","No","Internal"]
[null,null,null,24663,null,"120_3/22/2022 9:42:24 PM","2022-03-09T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","oil traces observed on main engine cylinder head.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","OIl leakage  source located and rectified.","2022-04-08T23:59:35","","Completed","2022-03-23T23:59:35","No","No","No","Internal"]
[null,null,null,24664,null,"120_3/22/2022 8:47:19 PM","2022-03-09T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","no.3 DG jacket cooling f.w. temp. sensor faulty","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","",""," Sensor changed ,working satisfactorily.","2022-04-08T23:59:35","","Completed","2022-03-17T23:59:35","No","No","No","Internal"]
[null,null,null,24651,null,"120_3/22/2022 9:58:23 PM","2022-03-10T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","oil leakages from aft seal leakages rectification.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","leakages rectification will be carried out with follow up with office. Aft Seal Fwd Seal to be renewed during dry dock. At present the water ingress is minimal. DEFFERRED TO DD","2023-06-23T23:59:35","","Completed","2023-05-28T23:59:35","Yes","No","No","Internal","As per maker's advise seal no #3S already put into use. System water ingress being drained regularly, very minimum oil loss. Vessel to raise DD spec in REFMAN for renewal of seal. DD will be in the year July 2025."]
[null,null,null,24653,null,"120_3/22/2022 8:33:43 PM","2022-03-13T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","manouvering platform auto and sound powered telephone out of operation","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","Auto telephone rectified, new sound  power telephone install","2022-04-22T23:59:35","","Completed","2022-04-22T23:59:35","No","No","No","Internal"]
[null,null,null,24654,null,"120_3/22/2022 9:39:29 PM","2022-03-17T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ballast and draft gauges found eratic/ faulty same to check and rectify.","Hull & Tanks","Cargo / Ballast Systems","Equipment Related","","","","","ballast tank no.1 to 5 port stbd both level sensors renewed with new spares, found readings moreover correspond with actual sounding with minor variation. Aft peak tank and Fore peak tank remote level gauge reading very much correspond with actual sounding, Forward and Aft draft gauges correspond with actual draft, Mid port and stbd draft gauges are erractic defective sensor. ","2022-12-22T23:59:35","SUNI220108","Completed",null,"No","No","No","Internal","Trust this job has already completed, kindly update accordingly."]
[null,null,null,24655,null,"120_3/22/2022 9:09:46 PM","2022-03-17T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","boiler damaged fuel oil hose with heater element to replace.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","Hose changed after receiving spares in Singapore.\nboiler tried out on Lsmgo ","2022-08-23T23:59:35","SUN 1220074","Completed","2022-08-11T23:59:35","No","No","No","Internal"]
[null,null,null,24641,null,"120_3/22/2022 9:05:24 PM","2022-05-10T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","all flouroscent light to be replace with LED lights","Miscellaneous","General Appearance","Equipment Related","","","","","ONGOIING ","2023-07-09T23:59:35","SUN1230008","Completed","2023-05-28T23:59:35","No","No","No","Internal","This job going on for last one year, please check & close out same asap. This is not a defect, kindly close out in DDRL."]
[null,null,null,26299,78297,"120_Sat Jul 16 2022 04:48:24 GMT+0800","2022-06-07T23:59:35","Defect","Ship Staff","Ship Staff Insp.","ECR alarm printer malfunctioning. Alarm activating frequently.","Elect. Mach. & Equip.","Cert. & Docu.","Equipment Related","","","","","ALARM PRINTER DATA CABLE CHANGED AND RESTARTED .","2022-12-22T23:59:35","","Completed","2022-11-02T23:59:35","No","No","No","Internal"]
[null,null,null,26303,63597,"120_Sat Jul 16 2022 05:47:45 GMT+0800","2022-06-07T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Hydroblaster Timer(on delay) malfunctioning. Not making contacts.","Deck - Machinery","Structural Condn. / WT integrity ","Equipment Related","","","","","vessel received spare hydroblaster in Singapore ","2022-08-23T23:59:35","SUN1220126","Completed","2022-08-12T23:59:35","No","No","No","Internal"]
[null,null,null,26300,49907,"120_Sat Jul 16 2022 04:57:08 GMT+0800","2022-06-10T23:59:35","Observation,Defect","Ship Staff","Ship Staff Insp.","No.2 Main Air Reservoir pressure transmitter defective.\nSensfail alarm.","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related","","","","","TRANSMITTER REPLACED WITH SPARE ONE","2022-08-23T23:59:35","SUN1220099","Completed","2022-08-16T23:59:35","No","No","No","Internal"]
[null,null,null,26294,60728,"120_Sat Jul 16 2022 01:26:17 GMT+0800","2022-06-26T23:59:35","Observation","Ship Staff","Ship Staff Insp.","EMBARKATION LADDER ON STBD SIDE LIFEBOAT DECK AND ONE FORWARD EMBARKATION LADDER IN BAD CONDITION.","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","TO BE REPLACED WITH NEW ONE. REQUISITION TO BE RAISED FOR SUPPLY AT SINGAPORE. Ladders received same replaced.","2022-12-23T23:59:35","","Completed","2022-11-05T23:59:35","No","No","No","Internal","Both ladders supplied, please check & confirm."]
[null,null,null,26295,87657,"0_Sat Jul 16 2022 01:27:55 GMT+0800","2022-06-26T23:59:35","Observation","Ship Staff","Ship Staff Insp.","ONE OF THE FIREMAN OUTFIT'S PANT WAS FOUND IN BAD / TORN CONDITION.","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","TO BE REPLACED WITH NEW ONE. REQUISITION FOR THE SAME TO BE RAISED FOR SUPPLY AT SINGAPORE","2022-08-08T23:59:35","","Completed","2022-08-08T23:59:35","No","No","No","Internal"]
[null,null,null,26296,63335,"0_Sat Jul 16 2022 01:30:10 GMT+0800","2022-06-26T23:59:35","Defect","Ship Staff","Ship Staff Insp.","THE BRIDGE FRONT PANEL CLOCK DIMMER NOT WORKING","Miscellaneous","General Appearance","Equipment Related","","","","","REQUISITION FOR THE SPARE HAS BEEN RAISED . same received and fitted back new dimmer and PCB, the dimmer circuit is changed as per the new dimmer supplied.","2022-12-22T23:59:35","SUN1220112","Completed","2022-12-09T23:59:35","No","No","No","Internal","Spares will be arranged at Rotterdam."]
[null,null,null,26297,50604,"0_Sat Jul 16 2022 01:32:17 GMT+0800","2022-06-26T23:59:35","Critical Equipment","Ship Staff","Ship Staff Insp.","THE LCD AND CCU FAN RUNNING HOURS FOR BOTH ECDIS SHOWING OVERDUE FOR REPLACEMENT.","Navigation - ECDIS","Navigation","Equipment Related","","","","","ECDIS SERVICING CARRIED OUT AND LCD AND CCU FANS CHANGED BY SHORE TECNICIANS AT SINGAPORE.","2022-10-23T23:59:35","SUN1220147","Completed","2022-09-29T23:59:35","No","No","No","Internal"]
[null,null,null,26298,15452,"0_Sat Jul 16 2022 01:35:24 GMT+0800","2022-06-26T23:59:35","Observation","Ship Staff","Ship Staff Insp.","NO 1 HATCH COVER CHAIN IN BAD CONDITION.","Miscellaneous","Cargo / Ballast Systems","Equipment Related","","","","","THE CHAIN TO BE CHIPPED AND MEASURE THE THICKNESS. IF THIN DOWN MORE THAN THE RECOMMENDED LIMIT, WILL BE REPLACING WITH NEW SPARE CHAIN ONBOARD.","2022-07-22T23:59:35","","Completed","2022-08-01T23:59:35","No","No","No","Internal"]
[null,null,null,26728,61792,"120_Fri Aug 19 2022 14:15:41 GMT+0800","2022-08-08T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Boiler salinometer defective, showing sensor fail.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","Boiler salinometer replaced with new spare, working satisfactory.","2022-12-08T23:59:35","SUN1220150","Completed","2022-11-22T23:59:35","No","No","No","Internal","Noted, will try to connect at Rotterdam."]
[null,null,null,27085,99507,"120_Fri Sep 16 2022 12:45:22 GMT+0800","2022-09-08T23:59:35","Observation,Defect","Ship Staff","Ship Staff Insp."," Main Fire pump overboard valve leaking from gland.\n","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Gland nuts eased up and gland tightened, leak stopped.","2022-12-08T23:59:35","","Completed","2022-10-19T23:59:35","No","No","No","Internal"]
[null,null,null,27685,48649,"120_Tue Sep 27 2022 07:57:32 GMT+0800","2022-09-09T23:59:35","Observation","Ship Staff","Ship Staff Insp.","OWS 15 ppm alarm display damaged., cannot see display ppm value properly.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Spare received  CPU card changed, OWS tried out.","2022-12-09T23:59:35","RO no: SUN1220148","Completed","2022-09-29T23:59:35","No","No","No","Internal"]
[null,null,null,27684,75455,"0_Fri Nov 04 2022 03:09:15 GMT+0800","2022-10-24T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Main cooling sea water pump no.2 mech seal leaking","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","","","","","Main cooling sea water pump  overhauled, mech seal renewed.","2022-11-07T23:59:35","","Completed","2022-11-04T23:59:35","No","No","No","Internal"]
[null,null,null,27686,97919,"120_Fri Nov 04 2022 03:01:58 GMT+0800","2022-10-24T23:59:35","Critical Equipment","Ship Staff","Ship Staff Insp.","RESCUE BOAT davit accumulators inefficient, suspect bladder leak, nitrogen gas leak. needs replacement or overhaul.","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","Accumulators replaced and charged with Nitrogen, davit tried out on reserve power. ","2022-11-23T23:59:35","","Completed","2022-10-30T23:59:35","No","No","No","Internal"]
[null,null,null,27681,71632,"120_Tue Nov 15 2022 16:14:16 GMT+0800","2022-10-25T23:59:35","Defect","Ship Staff","Ship Staff Insp.","As informed by makers, both PORT/ST’BD FWD anodes got faulty. So the faulty anodes should be renewed with new ones during ship’s dry dock without fail.","Hull & Tanks","Structural Condn. / WT integrity ","Equipment Related","","","","","Deferred to DD","2025-09-24T23:59:35","","Completed","2023-05-28T23:59:35","Yes","No","No","Internal","Please raise DD spec in REFMAN. Next special survey will be July 2025."]
[null,null,null,27683,79809,"120_Fri Nov 04 2022 22:56:51 GMT+0800","2022-10-25T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Pneumatic emergency DO pump not working .","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Pump opened up ,eased up lubricated and turned by hand, .\nput back and tried out on air, now working properly.","2023-01-27T23:59:35","","Completed","2022-10-25T23:59:35","No","No","No","Internal"]
[null,null,null,27678,33093,"0_Tue Nov 15 2022 21:55:22 GMT+0800","2022-11-07T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Sewage treatment plant vacuum pump no.2 is leaking, need to investigate the leak and rectify.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Pump to be overhauled , mech seal to be replaced with new spare. Pump overhauled, found shaft corroded, same build up by welding, fitted new mech seal and lip seal, tried out pump, found satisfactory.","2023-01-07T23:59:35","","Completed","2022-12-26T23:59:35","No","No","No","Internal","This can be PSC detainable deficiency, please get this job completed & update asap."]
[null,null,null,27679,81440,"120_Tue Nov 15 2022 21:29:02 GMT+0800","2022-11-07T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Sewage treatment plant is having a soft patch near the float area/flange in the sterilization tank.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Sewage treatment plant soft patch cropped, and newly fabricated plate welded, found satisfactory.","2023-02-07T23:59:35","","Completed","2022-11-17T23:59:35","No","No","No","Internal","Send us job plan & RA, hot work permit for repair sewage tank."]
[null,null,null,27682,79095,"120_Tue Nov 15 2022 21:53:32 GMT+0800","2022-11-07T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Fresh water generator ejector pump discharge pipe is holed, need to fabricate new pipe section.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Ejector pump discharge pipe removed from location, same welded and fitted back the same pipe. no leakage observed.","2022-12-07T23:59:35","","Completed","2022-11-19T23:59:35","No","No","No","Internal","Please take the opportunity of this anchorage & get the job completed."]
[null,null,null,27981,39706,"120_Sat Dec 03 2022 01:03:21 GMT+0800","2022-11-24T23:59:35","Defect","Ship Staff","Ship Staff Insp.","BWTS filter top cover sea water leakage from backflushing motor shaft.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","BWTS filter top cover to be overhauled, investigate the sea water leak from shaft seal and rectify the same. BWTS filter top cover overhauled, gear motor and assembly pulled out, found carbon bush wear down, same replaced with fabricated bronze bush, same tried out during operation, found satisfactory.","2023-02-22T23:59:35","","Completed",null,"No","No","No","Internal","Guideline send to vessel, please follow up for further assistance if deem necessary."]
[null,null,null,27982,41764,"120_Sat Dec 03 2022 00:56:42 GMT+0800","2022-11-24T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","Main fire pump no.2 Mechanical seal is leaking.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","","","","","Main fire pump no.2 to be overhauled, mech seal to be renewed. same was overhauled, mech seal renewed, bearing bush renewed, bottom impeller renewed.","2023-01-23T23:59:35","","Completed","2022-11-26T23:59:35","No","No","No","Internal","Kindly complete this job before arrival Rotterdam, can be proven as showstopper during PSC inspection."]
[null,null,null,27983,71208,"120_Sat Dec 03 2022 00:59:49 GMT+0800","2022-11-24T23:59:35","Defect","Ship Staff","Ship Staff Insp.","220 Volts low insulation due to Electrical deck sockets on deck.","Deck - Pipe / Fittings,Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","Several deck electrical socket fittings are in a bad shape, damaged, same to be replaced with new spare.SUN1230007 requisition Quarterly Electrical stores March 2023 raised.","2023-03-23T23:59:35","","Completed","2023-03-25T23:59:35","No","No","No","Internal","Need to complete this job on priority, can be detained by any third party inspection."]
[null,null,null,20459,null,"120_7/25/2021 4:54:52 PM","2022-11-24T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Ship Staff Insp.","HOLE IN THE DIFFUSER OF THE BILGE EDUCTOR PUMP","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","","","","","TEMPORARY COVER THE HOLE WITH PLASTIC STEEL(CORCOBOND)","2023-02-22T23:59:35","SUN1210029","Completed","2023-03-25T23:59:35","No","No","No","Internal","Spare already supplied to vessel, please check & renew same."]
[null,null,null,27673,96254,"0_Fri Nov 04 2022 03:25:01 GMT+0800","2022-11-25T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Incinerator secondary burner blower motor found burnt, same to be replaced with new spare.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Incinerator secondary burner blower motor to be replaced once new spare recieved.","2023-04-14T23:59:35","SUN1220197","Completed","2023-03-19T23:59:35","No","No","No","Internal","Spare motor will be connected at NPOC."]
[null,null,null,27677,94153,"0_Tue Nov 15 2022 21:58:16 GMT+0800","2022-12-07T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Bonding cable for pipe trunk laid up on deck is found missing at some location, the securing points for the cable is rusted or sheared off.","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","External Factors","","","","","securing point to be refurbished and new bonding cable to be used.","2023-02-07T23:59:35","","Completed","2023-02-21T23:59:35","No","No","No","Internal","Kindly get this job done asap & update."]
[null,null,null,28246,11531,"0_Tue Jan 03 2023 16:42:07 GMT+0800","2022-12-24T23:59:35","Observation","Ship Staff","Suptd. Insp.","During PSC inspection it was found CO2 room exhaust blower was not operational.","Critical Equip.","Safety / LSA / FFA","Equipment Related","","","","","The extraction blower in CO2 room need to be removed from place and check for its operation, same carried out, found blower impeller stuck, same replaced with spare ventilation blower.","2023-01-25T23:59:35","","Completed","2022-12-24T23:59:35","No","No","No","Internal","RO to raise for new blower of correct capacity & to installed"]
[null,null,null,28247,95471,"0_Tue Jan 03 2023 16:47:12 GMT+0800","2022-12-24T23:59:35","Observation","Ship Staff","Ship Staff Insp.","A class C fire door in electrical spare part room/workshop was kept inaccessible, also the door lock and handle was found to be missing.","Miscellaneous","Eng. / Strg. Comp.","Human Error","","","","","The door lock and handle was replaced, also the area around the door was cleared and made accessible. Post inspection the door handle door lock were fitted back in place, also the area was cleared for easy access.","2023-01-25T23:59:35","","Completed","2022-12-24T23:59:35","No","No","No","Internal","Door job already completed, kindly update DDRL &accordingly."]
[null,null,null,28248,86383,"120_Tue Jan 03 2023 16:35:44 GMT+0800","2022-12-24T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Manual call point in dry provision store is not operational, found during PSC inspection. same recorded as an observation by PSC inspector.","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","Manual call point at dry provision store to be replaced immediately as it was found during PSC inspection at Rotterdam, same rectified. Post inspection manual call point replaced, tried out found satisfactory.","2023-01-25T23:59:35","","Completed","2022-12-24T23:59:35","No","No","No","Internal","Already rectified, kindly update accordingly."]
[null,null,null,29276,27164,"120_Mon Jan 16 2023 16:32:26 GMT+0800","2023-01-11T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Aux engine no.2 jacket water common outlet pipe leaky blank flange, weak signal.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Leaky blank flange gasket  renewed.","2023-01-26T23:59:35","","Completed","2023-02-13T23:59:35","No","No","No","Internal"]
[null,null,null,29273,85427,"120_Mon Jan 16 2023 16:36:46 GMT+0800","2023-01-26T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Main engine jacket water cooler leaking.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Main engine jacket water HT cooler, is found to be leaking when not in operation, when the system cools down, likely the rubber gaskets shrink and cooler leaks with minimum. New gaskets to be procured and changed..Now No leaks","2023-04-25T23:59:35","","Completed","2023-04-24T23:59:35","No","No","No","Internal","Please check & advise from where the leakages are? Also advise RO no's, don't find any RO raised by vessel."]
[null,null,null,27086,14494,"120_Fri Sep 16 2022 12:51:49 GMT+0800","2023-02-08T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Fire and GS pump discharge valve to fire line leaking.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Valve to replaced at convenient/earliest opportunity. Ship staff have reconditioned one valve with lapping, but not up to the required standard.  valve will be done DD.","2023-05-07T23:59:35","","Completed","2023-05-11T23:59:35","No","No","No","Internal","Please check as spares already connected to vessel & complete the job."]
[null,null,null,26302,33789,"120_Sat Jul 16 2022 05:51:42 GMT+0800","2023-02-09T23:59:35","Defect","Ship Staff","Ship Staff Insp.","BWTS AFU Outlet pressure transmitter malfunctioning.Steady Current measured.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","Requisition raised  the same. Vessel recd Spares/","2023-05-07T23:59:35","SUN1220126","Completed","2023-05-11T23:59:35","No","No","No","Internal","Already spares connected to vessel, please check & rectify the defect. Close DDRL accordingly."]
[null,null,null,29275,51914,"120_Wed Mar 08 2023 17:13:07 GMT+0800","2023-02-20T23:59:35","Defect","Ship Staff","Ship Staff Insp.","F.W Hydrophore Pressure Switch is malfunctioning.  F.W Pump is running continuously.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","","","","","Requisition Raised.  Monitoring Pump.","2023-03-22T23:59:35","SUN1230064","Completed","2023-03-20T23:59:35","No","No","No","Internal"]
[null,null,null,29274,21321,"120_Tue Mar 07 2023 22:39:33 GMT+0800","2023-02-21T23:59:35","Breakdown,Observation","Ship Staff","Ship Staff Insp.","Main Engine Auto Backwash filter Not operational in Auto mode. ","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","manual flushing continues. vessel is under watch keeping","2023-03-26T23:59:35","sun1230048","Completed","2023-03-24T23:59:35","No","No","No","Internal"]
[null,null,null,27674,23914,"0_Fri Nov 04 2022 03:07:16 GMT+0800","2023-04-19T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Fresh water generator salinometer defective.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","This is for Faulty Salinometer , and other defect for faulty solenoid vv. RO ref no is mentioned at assigned place.\nJob completed, new spare salinometer received, same replaced.","2023-07-16T23:59:35","SUN1230016. Item4","Completed","2023-06-17T23:59:35","No","No","No","Internal","Awaiting for order confirmation from owner, will arrange at next covenient port after Ust Luga."]
[null,null,null,29998,51143,"120_Mon May 15 2023 00:43:35 GMT+0800","2023-05-27T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Main Air Compressor Unloader is Leaking .","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related","","","","","Tried after cleaning the inside parts but no success , Awaiting for Spares for OH or renewal . Unloader for Main air compressor no.1 replaced with new spare, found working satisfactory.","2023-07-26T23:59:35","SUN1230071","Completed","2023-07-13T23:59:35","No","No","No","Internal","Will try to connect spares at Singapore next call."]
[null,null,null,31335,60091,"0_Tue Jun 20 2023 22:19:44 GMT+0800","2023-06-16T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Deck machineries greasing routine not carried out diligently.","Deck - Machinery","Mooring","Behaviour Based","","","","","All mooring winches , hatch covers , RB davit , Lubricated.","2023-07-20T23:59:35","","Completed","2023-06-20T23:59:35","No","No","No","Internal"]
[null,null,null,31336,17719,"0_Tue Jun 20 2023 22:21:07 GMT+0800","2023-06-16T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Housekeeping is poor","Miscellaneous","General Appearance","Behaviour Based","","","","","All deck and Accommodation stores arranged.","2023-07-18T23:59:35","","Completed","2023-06-18T23:59:35","No","No","No","Internal"]
[null,null,null,31338,69179,"0_Tue Jun 20 2023 21:51:38 GMT+0800","2023-06-16T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Main engine fuel oil backwash filter automatic operation is restricted. Currently fuel is flushed manually in 4 hr interval. Drain valve is leaking.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Auto back wash filter bottom drain valve to be overhauled, further investigation to be carried out. Air piston operated valve opened up, changed seal ring, position of bottom drain valve solenoid valve put back to original 5/2 position.","2023-07-18T23:59:35","","Completed","2023-07-01T23:59:35","No","No","No","Internal"]
[null,null,null,31339,66282,"0_Tue Jun 20 2023 20:23:35 GMT+0800","2023-06-16T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Main cooling sea water pump performance is dropped ","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","","","","","Main cooling sea water pump no.1 to be overhauled and investigate the reason behind drop in performance. Main cooling sea water pump overhauled , wear rings replaced with new spare. Pump tried out, found satisfactory, mechanical seal to be replaced, minor leaks, seal height adjusted, pump tried out with no leaks observed.","2023-06-25T23:59:35","SUN1230172 MAIN SEA WATER COOLING PUMP","Completed","2023-07-08T23:59:35","No","No","No","Internal"]
[null,null,null,31340,24889,"0_Tue Jun 20 2023 21:25:56 GMT+0800","2023-06-16T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Ballast pump no.1 performance is reduced compared to Ballast pump no.2.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","","","","","Ballast pump no.1 to be overhauled and investigate the drop in performance. Pump overhauled, renewed wear rings, impeller replaced with new spare. Pump casing found damaged, same built up with devcon putty, pump tried out, performance found as  per capacity.","2023-07-18T23:59:35","","Completed","2023-07-08T23:59:35","No","No","No","Internal"]
[null,null,null,31337,32933,"120_Thu Jun 29 2023 23:33:29 GMT+0800","2023-06-27T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Fresh water generator ejector pump discharge line is holed near pump area.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Pipeline to be dismantled, section of the pipeline to be renewed. permanent repair to be carried out. Pipeline section disconnected, welding repair carried out, tried out found satisfactory.","2023-07-04T23:59:35","","Completed","2023-07-05T23:59:35","No","No","No","Internal"]
[null,null,null,null,64481,"120_Mon Jan 16 2023 16:30:15 GMT+0800","2023-07-11T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Fresh water generator bottom cover is holed.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Temporary repair work carried out, would recommend to off land the item at convenient port, get it fabricated from shore workshop with rubber coating and fit it back. Bottom shell cover replaced with new spare, found satisfactory.","2023-11-11T08:00:00","SUN1230038","Completed","2023-08-11T08:00:00","No","No","No","Internal","Same already fabricated locally in China, will be connected at next convenient port."]
[null,null,null,null,24591,"0_Tue Nov 15 2022 21:31:32 GMT+0800","2023-07-07T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Fresh water generator  Salinity Solenoid valve to be replaced with new valve.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Vessel rectified and replaced the solenoid valve.","2023-10-07T08:00:00","SUN1230098","Completed","2023-09-14T08:00:00","No","No","No","Internal","Duplicate reporting, please close out this in DDRL"]
[null,null,null,null,65298,"120_Thu Sep 21 2023 15:31:24 GMT+0800","2023-09-20T08:00:00","Breakdown","Ship Staff","Ship Staff Insp.","DURING OPERATION OF HATCH COVER 1 CONNECTING TURNBUCKLE WAS BROKEN AND VESSEL WAS UNABLE TO CLOSE HATCH COVER TILL THE TIME OF REPAIR (ABOUT 1 HR)","Deck - Machinery","Structural Condn. / WT integrity ","Equipment Related","","","","","IMMEDIETALY REPLACED WITH SPARE TURN BUCKLE AND CHAINS TIGHTENED EVENLY FOR SMOOTH OPERATION","2023-09-20T08:00:00","","Completed","2023-09-20T08:00:00","No","No","No","Internal"]
[null,null,null,null,68153,"120_Mon Oct 02 2023 16:07:33 GMT+0800","2023-09-16T08:00:00","Non Conformity","Owner / Marine / Tech. Suptd.","ISPS Audit","Door on funnel deck was left open while transtiting HRA","Miscellaneous","ISPS Related","Knowledge Based","","","","","Corrective Action: Door closed and briefed all crew and officer the consequences of security breach.\nPreventive Action: Brief/discuss the consequences of the security breach and security measure to be strictly implemented and follow accordingly on upcoming safety meeting.\n","2023-12-16T08:00:00","","Completed","2023-09-30T08:00:00","No","No","No","Internal"]
[null,null,null,null,36329,"0_Mon Oct 02 2023 16:09:53 GMT+0800","2023-09-16T08:00:00","Observation","Owner / Marine / Tech. Suptd.","ISPS Audit","FW filling pipes on poop deck to be pad locked to prevent contamination.","Miscellaneous","ISPS Related","Knowledge Based","","","","","Corrective Action: Advised to Officer in charged to keep pad locked the FW filling pipes at all times.\nPreventive Action: Brief/discuss the consequences of not putting pad locked in upcoming Safety Meeting to implement proper rounds, monitoring and supervision of all the FW filling pipes and prevent any contamination.\n","2023-12-16T08:00:00","","Completed","2023-09-30T08:00:00","No","No","No","Internal"]
[null,null,null,null,41896,"0_Mon Oct 02 2023 16:12:36 GMT+0800","2023-09-16T08:00:00","Observation","Owner / Marine / Tech. Suptd.","Nav Audit / Verification","Stering gear gyro heading misaligned by 10 degrees. ","Miscellaneous","Eng. / Strg. Comp.","Human Error","","","","","Corrective Action: Advised to officer on duty to realign the Steering Gear Gyro heading to the Master Gyro Heading accordingly.\nPreventive Action: Briefed/discussed to all OOW to thoroughly check the Bridge Pre-dep/Arrival Checklist and include Steering Gyro repeater heading check every noon at sea and log in the deck log book.\n","2023-12-16T08:00:00","","Completed","2023-09-30T08:00:00","No","No","No","Internal"]
[null,null,null,null,64633,"120_Mon Oct 02 2023 16:17:32 GMT+0800","2023-09-16T08:00:00","Observation","Owner / Marine / Tech. Suptd.","Engineering Audit","Emergency bilge valve numbered cable tie to be reeved thru spindle of valve not on the wheel itself for 100%compliance  ","Critical Equip.","Eng. / Strg. Comp.","Knowledge Based","","","","","Corrective Action: Instructed to Ch. Eng’r to change the securing arrange of the Emergency Bilge Valve to secured/reeved the numbered cable tie thru spindle of valve not on the wheel itself for 100% compliance to void question/issue onward inspection.\nPreventive Action: Brief/discuss to all Officer/Eng'r/Crew the consequence and 100% compliance and no chance of violation/issue onward inspection on upcoming safety meeting.\n","2023-12-16T08:00:00","","Completed","2023-09-30T08:00:00","No","No","No","Internal"]
[null,null,null,null,14982,"0_Mon Oct 02 2023 16:19:17 GMT+0800","2023-09-16T08:00:00","Observation","Owner / Marine / Tech. Suptd.","Engineering Audit","OWS OB valve numbereed cable tie to be reeved thru spindle of valve not on the wheel itself for 100%compliance.","","Eng. / Strg. Comp.","","","","","","Corrective Action: Instructed to Ch. Eng’r to change the securing arrange of the OWS OB valve to secured/reeved the numbered cable tie thru spindle of valve not on the wheel itself for 100% compliance to void question/issue onward inspection.\nPreventive Action: Brief/discuss to all Officer/Eng'r/Crew the consequences and 100% compliance and no chance of violation/issue onward inspection on upcoming safety meeting.\n","2023-12-16T08:00:00","","Completed","2023-09-30T08:00:00","No","No","No","Internal"]
[null,null,null,null,80088,"120_Mon Oct 02 2023 16:21:30 GMT+0800","2023-09-16T08:00:00","Observation","Owner / Marine / Tech. Suptd.","Mooring Audit","Locking pins for all mooring winch gear handles - receptacles to be derusted and lanyards attached ","Deck - Mooring Machinery","Mooring","Knowledge Based","","","","","Corrective Action: Instructed to Ch. Off. to check and de-rust/repaint all Mooring winch gear handles locking pin receptacles and missing lanyards to be make and attached on the pin and winch engaging handle.\nPreventive Action: Brief/discuss to all officer/Eng'r/crew proper supervision, monitoring and maintenance as per PMS for strict compliance and the consequences on upcoming safety meeting.\n","2023-12-16T08:00:00","","Completed","2023-09-30T08:00:00","No","No","No","Internal"]
[null,null,null,null,91743,"0_Mon Oct 02 2023 16:29:07 GMT+0800","2023-09-16T08:00:00","Non Conformity","Owner / Marine / Tech. Suptd.","ISM Audit","all 4 gangway wire lashings were not rigged properly after departure S'pore - were found loose.","Deck - Machinery","ISM Related","Knowledge Based","","","","","Corrective Action: Instructed Bosun to double check and retighten/rigged properly and make sure all equipment in use such as gangway to proper secured and stowed every departure port prior finish work on deck.\nPreventive Action: Brief/discussed to all Officer/Eng'r/Crew proper securing and stowed of all deck machinery, equipment, gangway, stores and tools etc. to strictly implemented, consequence and risk associated left unproperly secured and stowed on upcoming safety meeting.\n","2023-12-16T08:00:00","","Completed","2023-09-30T08:00:00","No","No","No","Internal"]
[null,null,null,null,54401,"0_Mon Oct 02 2023 16:31:09 GMT+0800","2023-09-16T08:00:00","Non Conformity","Owner / Marine / Tech. Suptd.","ISM Audit","Bunkering in S'pore - Wilden pump was available but not keot in readiness with air / suction / discharge hoses connected.","Miscellaneous","ISM Related","Knowledge Based","","","","","Corrective Action: Instructed Bosun and Ch. Officer to kept the wilden pump with air/suction/discharge hoses connected in order during emergency is always ready to use just to open the air valve supply as time is essence and not losing time during emergency to content the spill right away. \nPreventive Action: Brief/discussed to all Officer/Eng'r/Crew the importance of every spill equipment to kept in readiness at all times and consequences and lapses will occur during the time of emergency arouse on upcoming safety meeting.\n","2023-12-16T08:00:00","","Completed","2023-09-30T08:00:00","No","No","No","Internal"]
[null,null,null,null,99180,"0_Mon Oct 02 2023 16:37:38 GMT+0800","2023-09-17T08:00:00","Observation","FSC Inspector","Flag State Insp.","Cooling water level of EM Generator was found insufficient. ","Critical Equip.","Emgcy. Systems","Behaviour Based","","","","","Vessel Comments: RECTIFIED BEFORE INSPECTOR DISEMBARKATION\nCorrective Action: Fill up the water in the cooling water system of EM Generator at a time observation noted by the inspector.\nPreventive Action: Brief/discuss on upcoming Safety Meeting to implement proper rounds, monitoring and supervision of all engine personnel to strictly adhere at all times. Any abnormality observed to rectify and report immediately to the head department.\n","2023-12-17T08:00:00","","Completed","2023-09-30T08:00:00","No","No","No","External"]
[null,null,null,null,77000,"0_Mon Oct 02 2023 16:39:35 GMT+0800","2023-09-17T08:00:00","Observation","FSC Inspector","Flag State Insp.","Found some safety pin of engage levers at the mooring winch aft not in place. ","Deck - Mooring Machinery","Mooring","Knowledge Based","","","","","Vessel Comments: RECTIFIED BEFORE INSPECTOR DISEMBARKATION\nCorrective Action: Check all engage lever safety pin of mooring winches drum forward/aft station and in place the safety pin in the correct position. Briefed/discussed to all deck crew & officers the consequences and the important of the safety pin to keep in place in correct position every after use of the mooring winches and strictly to adhere accordingly.\nPreventive Action: Briefed/discussed/Training to all deck crew & officers the consequences and the important of the safety pin to keep in place in correct position every after use of the mooring winches and strictly compliance. All officer advised after mooring operations to put in practice to double check the safety pin in place in the correct position prior living the station and keep remind everybody that safety pin of the mooring winches drum engage lever to be disengage and put safety pin in place always after every using the Mooring winches during tool box meeting carry out during mooring operations.\n","2023-12-17T08:00:00","","Completed","2023-09-30T08:00:00","No","No","No","External"]
[null,null,null,null,90971,"0_Mon Oct 02 2023 16:41:26 GMT+0800","2023-09-17T08:00:00","Observation","FSC Inspector","Flag State Insp.","- It was found that the correction pen was used to correct some details inside the bunker sample and SECA fuel-change over record book on 23 Sept 2021/ 26 Nov 2021/ 27 Nov 2021.","Documentation","Cert. & Docu.","Knowledge Based","","","","","Vessel Comments: This observation happened from previous management.\nCorrective Action/Preventive Action: Briefed/training/discussed to all Officer/Eng'r/Crew of the above observation not to be follow using of correction pen to correct some entries in all log books, just strike one or two lines on the corrected entry and signed.\n","2023-12-17T08:00:00","","Completed","2023-09-30T08:00:00","No","No","No","Internal"]
[null,null,null,null,14662,"0_Mon Oct 02 2023 16:46:15 GMT+0800","2023-09-17T08:00:00","Non Conformity","FSC Inspector","Flag State Insp.","The HFO vent head tank No. 02 & No. 03 Port Side were missing the rubber seals ","E/R - Pipes/ valves & fittings","Structural Condn. / WT integrity ","Behaviour Based","","","","","Vessel Comments: Rectified during the inspection\nCorrective Action: Put back the rubber seals upon noted the missing rubber seal during the inspection. Checked all other vents head tank rubber seals all found in place.\nPreventive Action: Brief/discussed to all officer/Eng'r/crew the consequences and importance/use of this rubber seal of to each compartment. Proper supervision and maintenance as per PMS & Maker's recommendation to strictly adhere accordingly.\n","2023-09-17T08:00:00","","Completed","2023-09-17T08:00:00","No","No","No","External"]
[null,null,null,null,48157,"120_Mon Oct 02 2023 16:48:10 GMT+0800","2023-09-17T08:00:00","Non Conformity","FSC Inspector","Flag State Insp.","The limit switch of rescue boat davit was found in frozen","Deck - Machinery","Safety / LSA / FFA","Equipment Related","","","","","Vessel Comments: Rectified during the inspection\nCorrective Action: Changed the defective limit switch with the new spare onboard, test on the present of Inspector and found satisfactory.\nPreventive Action: Brief/discussed to all Officer/Eng'r/Crew the consequences and the importance/purpose of the limit switch. Proper maintenance of all equipment as per PMS and Maker's guidelines to strictly adhere accordingly and to address to rectify all defective equipment and to report right away to the head department accordingly.\n","2023-09-17T08:00:00","","Completed","2023-09-17T08:00:00","No","No","No","External"]
[null,null,null,null,54282,"0_Mon Oct 02 2023 16:52:28 GMT+0800","2023-09-17T08:00:00","Non Conformity","FSC Inspector","Flag State Insp.","Found 01 chain supporting of hatch cover hold No. 02 FWD St. Bd damage. To be rectified before departure","Cargo Mach.","Safety / LSA / FFA","Equipment Related,Industry Issue,External Factors,Behaviour Based,Knowledge Based","","","","","Vessel Comments: It was damaged recent opening of the cargo hold No. 2 hatch and rectified before vessel sailed.\nRoot Cause: Lack of proper maintenance and Lack of Situational Awareness\nCorrective Action: Request hot work permit to Harbour master via Agent and same hot work permit approval requested to office. Cut the damaged chain supporting bracket and fabricated/welded/installed new chain supporting bracket.\nPreventive Action: Checked all other chain supporting bracket and replace if required. Brief/discussed to all Officer/Eng'r/Crew Proper maintenance as per PMS to strictly adhere accordingly and to address and rectify all defective equipment and to report right away to the head department accordingly.\n","2023-09-23T08:00:00","","Completed","2023-09-20T08:00:00","No","No","No","External"]
[null,null,null,null,28055,"0_Mon Oct 02 2023 16:54:32 GMT+0800","2023-09-17T08:00:00","Non Conformity","FSC Inspector","Flag State Insp.","The hydraulic jack of free fall lifeboat davit found leakage hydraulic oil. To be rectified within 30 days","LSA / FFA","Safety / LSA / FFA","Equipment Related,External Factors","","","","","Corrective Action: Notified Office and request shore’s personnel assistance to overhaul/dismantle and rectify the starboard side hydraulic Ram Seal leakage.\nPreventive Action: To overhaul/dismantle the other side of the hydraulic ram and replace new seal. Brief/discussed to all Officer/Eng'r/Crew Proper maintenance as per PMS and Maker Recommendation to strictly adhere accordingly. Be observance and report any abnormalities observed to the head department accordingly\n","2023-10-17T08:00:00","","Completed","2023-09-29T08:00:00","No","No","No","External"]
[null,null,null,null,51384,"0_Tue Oct 03 2023 16:41:05 GMT+0800","2023-09-27T08:00:00","Defect","Ship Staff","Ship Staff Insp.","#3 CH CONTROL BLOCK FOR HYDR JACK FOR HATCH COVER OPERATION LEAKING FROM BASE.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","RENEWED WITH NEW SPARE","2023-10-30T08:00:00","","Completed","2023-09-30T08:00:00","No","No","No","Internal"]
[null,null,null,null,48706,"0_Tue Oct 03 2023 19:35:39 GMT+0800","2023-10-01T08:00:00","Defect,Critical Equipment","Ship Staff","Ship Staff Insp.","MAIN ENGINE CONTROL AIR REDUCER LEAKAGE","E/R - Main Engine","Emgcy. Systems","Equipment Related","","","","","SAME OVERHAULED WITH SPARE GASKET AND PUT IN USE","2023-10-31T08:00:00","","Completed","2023-10-01T08:00:00","No","No","No","Internal"]
[null,null,null,null,88996,"0_Wed Oct 04 2023 09:31:06 GMT+0800","2023-09-30T08:00:00","Critical Equipment","Ship Staff","Ship Staff Insp.","AE2 PRIMING PUMP NOISY OPERATION","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","TO OVERHAUL OR RECTIFY THE FAULT","2023-10-30T08:00:00","","Completed","2023-10-03T08:00:00","No","No","No","Internal"]
[null,null,null,null,11324,"0_Mon Oct 02 2023 16:43:53 GMT+0800","2023-09-17T08:00:00","Observation","FSC Inspector","Flag State Insp.","No.2 Main seawater cooling pump was found slightly leakage.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","","","","","Corrective Action: Dismantling the No. 2 Main Seawater cooling pump and replace new spare onboard. Tested and no more leaks.\nPreventive Action: Brief/discuss to all engine personnel to upcoming Safety Meeting to adhere proper monitoring, checking and supervision of all machinery. Any observed leaks or abnormality to report and rectify right away. Proper maintenance as per PMS and Maker recommendation to strictly implemented accordingly.\n","2023-12-17T08:00:00","","Completed","2023-09-30T08:00:00","No","No","No","External"]
[null,null,null,null,10893,"0_Mon Oct 02 2023 16:27:04 GMT+0800","2023-09-16T08:00:00","Observation","Owner / Marine / Tech. Suptd.","MLC Audit","Few chair reksin covers found torn in off & crew smoke room. One chair in ECR back rest broken - dispose off the chair to prevent personal injury.","Accommodation","MLC Related","Knowledge Based","","","","","Corrective Action: Instructed bosun to fabricate new cover of the chair reksin covers torn in Off & Crew Smoke Room and disposed the chair in ECR with broken back rest.\nPreventive Action: Brief/discuss to all officer/Eng’r/crew the associated risk of the broken chair and bad impression on the torn covers in Officer and Crew Smoke Room on upcoming safety meeting.\n","2023-12-16T08:00:00","","Completed","2023-09-30T08:00:00","No","No","No","Internal"]
[null,null,null,null,89336,"0_Wed Oct 04 2023 09:26:58 GMT+0800","2023-09-30T08:00:00","Critical Equipment","Ship Staff","Ship Staff Insp.","FLYWHEEL BILGE ALARM NOT WORKING","Critical Equip.","Emgcy. Systems","Equipment Related","","","","","TO RECTIFY OR RENEW/ OVERHAULED AND TRIED OUT SATISFACTORY.","2023-12-30T08:00:00","","Completed","2023-10-07T08:00:00","No","No","No","Internal"]
[null,null,null,null,69546,"0_Tue Oct 03 2023 08:16:13 GMT+0800","2023-09-16T08:00:00","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Trolley for transporting O2 and Acetylene cylinders to be given a dnew look before it corrodes and wastes away.","Miscellaneous","General Appearance","Behaviour Based","","","","","DERUSTED AND PAINTED ","2023-10-15T08:00:00","","Completed","2023-10-04T08:00:00","No","No","No","Internal"]
[null,null,null,null,14133,"120_Tue Oct 03 2023 08:19:37 GMT+0800","2023-10-01T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Flexible hydraulic hose of Cylinder Fwd of No.3 Cargo hold leaking and to replace with new. ","Deck - Machinery","Cargo / Ballast Systems","Equipment Related","","","","","REPLACED WITH NEW HOSE ","2023-10-04T08:00:00","","Completed","2023-10-04T08:00:00","No","No","No","Internal"]
[null,null,null,null,77840,"0_Tue Oct 03 2023 07:24:02 GMT+0800","2023-09-16T08:00:00","Other","Owner / Marine / Tech. Suptd.","Bunkering Audit","All wilden pumps to be provided a wooden base - else the base stand will scratch and damage paint on deck. ","Miscellaneous","General Appearance","Behaviour Based","","","","","WOODEN BASE FOR WILDEN PUMPS FABRICATED ","2023-09-26T08:00:00","","Completed","2023-10-04T08:00:00","No","No","No","Internal"]
[null,null,null,null,46372,"0_Tue Oct 03 2023 13:12:04 GMT+0800","2023-09-28T08:00:00","Critical Equipment","Ship Staff","Ship Staff Insp.","FIRE AND BILGE PUMP NOT IN USE. ","E/R - Pumps","Cargo / Ballast Systems","Equipment Related","","","","","SAME TO BE TRIED OUT AND ROOT CAUSE OF NOT IN USE ASCERTAINED. TO BE OPENED FOR INSPECTION AND OVERHAULED.\nOVERHAULED WITH NEW SPARES AND ONLY MECH SEAL USED OLD, NO LEAKS","2023-11-30T08:00:00","","Completed","2023-10-06T08:00:00","No","No","No","Internal"]
[null,null,null,null,26961,"0_Wed Oct 04 2023 09:29:13 GMT+0800","2023-09-20T08:00:00","Defect","Ship Staff","Ship Staff Insp.","TRO STBD GIVING ALARM, FOUND RELIEF VALVES OF SAMPLING LINES FROZEN","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","OPENED AND OVERHAULED THE RELIEF VALVES AND BOXED BACK","2023-10-30T08:00:00","","Completed","2023-10-01T08:00:00","No","No","No","Internal"]
[null,null,null,null,58330,"0_Tue Oct 03 2023 07:47:12 GMT+0800","2023-09-16T08:00:00","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","The fwd mast Air horn oil to be changed and a record of oil change to be maintained on board. ","Navigation - Others","ISM Related","Equipment Related","","","","","OIL RENEWED AND JOB UPDATED IN PAL","2023-09-26T08:00:00","","Completed","2023-10-12T08:00:00","No","No","No","Internal"]
[null,null,null,null,15798,"0_Tue Jun 20 2023 20:16:58 GMT+0800","2023-07-16T08:00:00","Breakdown","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Fire and bilge pump is not operational, due to defective mechanical seal.","E/R - Pumps","Safety / LSA / FFA","Equipment Related","","","","","Fire and bilge pump to be overhauled, shaft trueness to be checked, mechanical seal to be renewed. Ship staff received spares in SIngapore Sept 23, job will be carried out at the earliest next opportunity. Currently Fire and GS pump is in operation and working satisfactory.","2023-10-18T08:00:00","SUN1230117 ","Completed","2023-10-06T08:00:00","No","No","No","Internal"]
[null,null,null,null,46116,"120_Mon Jul 17 2023 04:58:02 GMT+0800","2023-07-15T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Cooling fan for motors is defective","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","","","","","Various motors in Engine room have damaged cooling fan, making their use out of operation, new cooling fan to be procured. Vessel received spares, fan will be replaced as per job planning.\nCOMPLETED RENEWAL FOR 4 MOTORS.","2023-10-09T08:00:00","SUN1230176 COOLING FAN FOR VARIOUS MOTORS","Completed",null,"No","No","No","Internal","Vessel already received the cooling fans in Singapore, kindly replace & update DDRL."]
[null,null,null,null,72048,"120_Mon Jul 17 2023 04:54:26 GMT+0800","2023-08-15T08:00:00","Observation","Ship Staff","Ship Staff Insp.","Low insulation at 220V","Deck - Machinery","Emgcy. Systems","Equipment Related","","","","","Deck sockets, Air whistle, port and stbd pilot embarkation are found to be source for low insulation. Low insulation from deck sockets and port and stbd embarkation light is rectified, pending is from Air whistle.","2023-10-15T08:00:00","","Completed","2023-10-14T08:00:00","No","No","No","Internal","Please complete this job at Vietnam anchorage & update DDRL."]
[null,null,null,null,79932,"0_Tue Oct 03 2023 16:38:16 GMT+0800","2023-09-26T08:00:00","Defect","Ship Staff","Ship Staff Insp.","#2 CH CHAIN ROLLER WHEEL BEARING BROKEN","Cargo Mach.","Structural Condn. / WT integrity ","Equipment Related","","","","","TO RENEW BEARINGS","2023-12-30T08:00:00","","Completed","2023-10-16T08:00:00","No","No","No","Internal"]
[null,null,null,null,91428,"0_Tue Oct 03 2023 16:36:51 GMT+0800","2023-09-26T08:00:00","Defect","Ship Staff","Ship Staff Insp.","#3 CH STAFFA MOTOR SEAL LEAKING","Cargo Mach.","Structural Condn. / WT integrity ","Equipment Related","","","","","TO RENEW SEAL AND FABRICATED SEAL COVER","2023-12-30T08:00:00","","Completed","2023-10-14T08:00:00","No","No","No","Internal"]
[null,null,null,null,57830,"120_Thu Oct 19 2023 09:37:13 GMT+0800","2023-10-11T08:00:00","Defect","Ship Staff","Ship Staff Insp.","LEAKAGE IN VALVE CONTROL HYDRAULIC LINE AT PORT SIDE NEAR MIDSHIP STORE. ","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","","","","","LEAKAGE LOCATED , LINE CUT  AND INSTALLED HIGH PRESSURE COUPLING (ARMATO) ","2023-10-20T08:00:00","","Completed","2023-10-18T08:00:00","No","No","No","Internal"]
[null,null,null,null,19556,"0_Tue Oct 03 2023 07:41:20 GMT+0800","2023-09-16T08:00:00","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","MOT gangway - found lashed with Nylon rope - recommend use railing support , wire snotters and bottle screws and lash the MOT gangway vertically using eye pads provided. ","Deck - Machinery","General Appearance","Inappropriate Procedure","","","","","LASHINGS TAKEN WITH WIRE AND TURN BUCKLES","2023-11-15T08:00:00","","Completed","2023-10-14T08:00:00","No","No","No","Internal"]
[null,null,null,null,66151,"0_Tue Oct 03 2023 19:25:31 GMT+0800","2023-09-29T08:00:00","Critical Equipment","Ship Staff","Ship Staff Insp.","AE 1 LO LOW PRESSURE TRIP NOT FUNCTIONAL","Critical Equip.","Emgcy. Systems","Equipment Related","","","","","SENSOR PROBLEM RECTIFIED.NOW WORKING SATISFACTORILY.","2023-12-30T08:00:00","","Completed","2023-10-16T08:00:00","No","No","No","Internal"]
[null,null,null,null,21187,"0_Tue Oct 03 2023 19:22:22 GMT+0800","2023-09-29T08:00:00","Defect,Critical Equipment","Ship Staff","Ship Staff Insp.","AE 1 JKT FW HIGH TEMPERATURE  TRIP NOT FUNCTIONAL","Critical Equip.","Safety / LSA / FFA","Equipment Related","","","","","SESNOR PROBLEM RECTIFIED. NOW WORKING SATISFACTORILY.","2023-12-30T08:00:00","","Completed","2023-10-16T08:00:00","No","No","No","Internal"]
[null,null,null,null,54047,"0_Tue Oct 03 2023 08:10:50 GMT+0800","2023-09-16T08:00:00","Observation","Owner / Marine / Tech. Suptd.","MLC Audit","Deep freezer for stowing wet garbage to be commissioned. ","Miscellaneous","MLC Related","Equipment Related","","","","","DEEP FREZZER INSTALLED IN PROVISION STORE. ARMOURED CABLE USED FOR POWER SUPPLY AND CABLE SECURED.","2023-12-10T08:00:00","","Completed","2023-10-19T08:00:00","No","No","No","Internal"]
[null,null,null,null,97010,"0_Tue Oct 03 2023 19:33:51 GMT+0800","2023-09-30T08:00:00","Critical Equipment","Ship Staff","Ship Staff Insp.","EMG FIRE PUMP PRIMING UNIT CLUTCH DAMAGED, ENGAGING LEVER SEIZED, CLUTCH WORN OUT","Critical Equip.","Emgcy. Systems","Equipment Related","","","","","TO RENEW WITH SPARE. CLUTCH MECHANISM FREED, NEW CLUTCH FITTED, BEARINGS ARE WRONG SUPPLY.\nNOW WORKING SATISFACTORILY.","2023-12-30T08:00:00","","Completed","2023-10-14T08:00:00","No","No","No","Internal"]
[null,null,null,null,31267,"0_Tue Oct 03 2023 06:51:07 GMT+0800","2023-09-16T08:00:00","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Hydraulic oil type for windlass + hatch opening mahinery to be stencilled on the Tank to ensure no mistake is made. Also one 200 ltr oil drum to be kept in vicinity for immediate replenishment. ","Deck - Machinery","ISM Related","Equipment Related","","","","","Stencilled Correct type of Oil to be used .  Spare kept","2023-10-26T08:00:00","","Completed","2023-10-21T08:00:00","No","No","No","Internal"]
[null,null,null,null,27799,"120_Mon Oct 09 2023 12:17:50 GMT+0800","2023-09-18T08:00:00","Defect","Ship Staff","Ship Staff Insp.","BOTTOM FLOOR PLATES FASTENING SCREWS ARE REMOVED FROM SEVERAL PLATES.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","TO SCREW AND FASTEN PROPERLY ALL PLATES ON BOTTOM PLATFORM","2023-12-31T08:00:00","","Completed","2023-10-22T08:00:00","No","No","No","Internal"]
[null,null,null,null,69074,"0_Tue Oct 10 2023 10:26:59 GMT+0800","2023-09-27T08:00:00","Defect","Ship Staff","Ship Staff Insp.","FW HYDROPHORE TANK AND SYSTEM NOT IN USE AND CAUSE UNKNOWN","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","TO CHECK BOTH DW PUMPS AND OPEN TANK FOR INSPECTION, PUT IN USE AND CHECK PROPER FUNCTIONING","2023-12-26T08:00:00","","Completed",null,"No","No","No","Internal"]
[null,null,null,null,42775,"0_Mon Oct 09 2023 12:20:33 GMT+0800","2023-09-18T08:00:00","Defect","Ship Staff","Ship Staff Insp.","SOME ANTISPLASH TAPES FOR HP PIPES NOT IN PLACE AND A FEW OPENING WITH HEAT","Critical Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","TO RENEW AND SEAL ALL HP OIL JOINTS WITH ANTISPLASH TAPE","2023-12-31T08:00:00","","Completed",null,"No","No","No","Internal"]
[null,null,null,null,92488,"120_Sun Oct 22 2023 16:45:40 GMT+0800","2023-09-17T08:00:00","Critical Equipment","Ship Staff","Ship Staff Insp.","EMG FIRE PUMP PRIMING DEVICE NOT OPERATIONAL.","Critical Equip.","Emgcy. Systems","Equipment Related","","","","","OVERHAULED AND MADE OPERATIONAL","2023-10-22T08:00:00","","Completed","2023-10-22T08:00:00","No","No","No","Internal"]
[null,null,null,null,47762,"120_Sun Oct 22 2023 17:23:19 GMT+0800","2023-09-17T08:00:00","Critical Equipment","Ship Staff","Ship Staff Insp.","MAIN SW PUMP NO 1 NOT FUNCTIONAL, CASING DAMGED","Critical Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","TO RENEW CASING AND OVERHAUL FULL PUMP AFTER CHECKING FOR ANY DAMAGE TO OTHER COMPONENTS","2023-12-19T08:00:00","","Completed","2023-10-17T08:00:00","No","No","No","Internal"]
[null,null,null,null,25769,"120_Mon Oct 02 2023 16:35:15 GMT+0800","2023-09-17T08:00:00","Observation","FSC Inspector","Flag State Insp.","The person assigned to muster at that station have not sufficient space as per SOLAS 1996-1998/chapter III/ Reg.11 requirement, at least 0.35m2 per person.\n","Miscellaneous","Safety / LSA / FFA","Knowledge Based","","","","","Corrective Action: Repaint and Re-stencil the muster station as per the requirements. Briefed and explained to the person in-charge the required requirements as per SOLAS 1996-1998/chapter III/ Reg.11 requirement, at least 0.35m2 per person. \nPreventive Action: Briefing to all officer/Crew of the said observation and requirements for awareness and compliance.\n","2023-12-17T08:00:00","","Completed","2023-10-21T08:00:00","No","No","No","External"]
[null,null,null,null,94014,"0_Mon Oct 02 2023 16:25:19 GMT+0800","2023-09-16T08:00:00","Observation","Owner / Marine / Tech. Suptd.","Cargo Audit","Emergency Hatch opening  pump/motor to be included in PMS  ","Deck - Machinery","Cargo / Ballast Systems","Equipment Related","","","","","Checked PMS found testing of Emergency Hatch Opening pump/motor exist in vessel PMS. Tried out and Carried Out Training of the emergency operations to all crew.","2023-12-16T08:00:00","","Completed","2023-10-20T08:00:00","No","No","No","Internal"]
[null,null,null,null,69599,"0_Tue Oct 03 2023 19:41:41 GMT+0800","2023-10-03T08:00:00","Defect","Ship Staff","Ship Staff Insp.","REMOTE HYDRAULIC VALVE PIPES FOUND CORRODED AND LEAKING IN SOME PLACES.","Deck - Machinery","Cargo / Ballast Systems","Equipment Related","","","","","SAME TO BE RECTIFIED AND LEAKS ARRESTED","2023-12-30T08:00:00","","Completed","2023-10-18T08:00:00","No","No","No","Internal"]
[null,null,null,null,80401,"0_Tue Oct 03 2023 08:05:02 GMT+0800","2023-09-16T08:00:00","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","To Keep on bridge , Canvass bag stencilled SART / EPIRB for carrying during abandon ship drill and in case of emergencies ","LSA / FFA","Safety / LSA / FFA","Knowledge Based","","","","","Fabricate Canvass bag for same.","2023-10-15T08:00:00","","Completed","2023-10-15T08:00:00","No","No","No","Internal"]
[null,null,null,null,40358,"0_Tue Oct 03 2023 07:20:16 GMT+0800","2023-09-16T08:00:00","Other","Owner / Marine / Tech. Suptd.","Bunkering Audit","Sighted 3 wilden pumps in Bosun store- prepare one wilden pump each for port and stbd bunkering times. Each fitted with its own air ,suction and discharge hoses. and positioned close to ship side and mark a square in deck stencilled \" WILDEN PUMP AREA\" discharge hoses to be emptied into SOPEP OIL SPILL DRUMS. ","Miscellaneous","MARPOL Related","Behaviour Based","","","","","Stencilled \"WILDEN PUMP AREA\" and training carried out.","2023-09-26T08:00:00","","Completed","2023-10-15T08:00:00","No","No","No","Internal"]

{"sheet":"Calc","index":2,"n_rows":28,"n_cols":12,"rows_kept":28,"cut":false,"hidden":true,"merged":[]}
["Def_type","Def_cause","Equipments","VIQrefno","Observer_code"]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,"Dim itemSele As Long"]
[null,null,null,null,null,null,null,null,null,null,null,"   dim startRow as integer"]
[null,null,null,null,null,null,null,null,null,null,null,"   startRow=1"]
[null,null,null,null,null,null,null,null,null,null,null,"        For itemSele = 0 To ListBox1.ListCount - 1"]
[null,null,null,null,null,null,null,null,null,null,null,"        If ListBox1.Selected(itemSele) = True Then"]
[null,null,null,null,null,null,null,null,null,null,null,"        Worksheets(\"WorksheetName\").Range(\"A\" & startRow).Value = ListBox1.List(itemSele)"]
[null,null,null,null,null,null,null,null,null,null,null,"        startRow = startRow + 1"]
[null,null,null,null,null,null,null,null,null,null,null,"        End If"]
[null,null,null,null,null,null,null,null,null,null,null,"        Next"]
[null,null,null,null,null,null,null,null,null,null,null,"Dim LastRowA As String"]
[null,null,null,null,null,null,null,null,null,null,null,"        Dim itemSele As Long"]
[null,null,null,null,null,null,null,null,null,null,null,"       Dim startRow as integer"]
[null,null,null,null,null,null,null,null,null,null,null,"        LastRowA = ActiveSheet.Cells(Rows.count, \"A\").End(xlUp).row"]
[null,null,null,null,null,null,null,null,null,null,null,"        startQue = 0"]
[null,null,null,null,null,null,null,null,null,null,null,"        For itemSele = 0 To ListBox1.ListCount - 1"]
[null,null,null,null,null,null,null,null,null,null,null,"        For startRow = 1 To LastRowA"]
[null,null,null,null,null,null,null,null,null,null,null,"        If Worksheets(\"WorksheetName\").Range(\"A\" & startRow).Value = ListBox1.List(itemSele) Then"]
[null,null,null,null,null,null,null,null,null,null,null,"        ListBox1.Selected(itemSele) = True"]
[null,null,null,null,null,null,null,null,null,null,null,"        Exit For"]
[null,null,null,null,null,null,null,null,null,null,null,"        End If"]
[null,null,null,null,null,null,null,null,null,null,null,"        Next j"]
[null,null,null,null,null,null,null,null,null,null,null,"        Next"]
[null,null,null,null,null,null,null,null,null,null,null,"        End If"]

{"sheet":"Areaofobs","index":3,"n_rows":17,"n_cols":2,"rows_kept":17,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Cargo / Ballast Systems",11]
["Cert. & Docu.",2]
["Communication",6]
["Crew Management",3]
["Emgcy. Systems",13]
["Eng. / Strg. Comp.",14]
["General Appearance",15]
["Ice Opns.",17]
["ISM Related",7]
["ISPS Related",10]
["MARPOL Related",9]
["MLC Related",4]
["Mooring",12]
["Navigation",5]
["Safety / LSA / FFA",8]
["Structural Condn. / WT integrity ",16]

{"sheet":"Vessel_type","index":4,"n_rows":1,"n_cols":2,"rows_kept":1,"cut":false,"hidden":true,"merged":[]}
["Vessel_type","ID"]

{"sheet":"Deficiency_type","index":5,"n_rows":8,"n_cols":3,"rows_kept":8,"cut":false,"hidden":true,"merged":[]}
["TITLE","Type of deficiency_description","ID"]
["Breakdown",null,6]
["Critical Equipment",null,4]
["Defect",null,1]
["Guarantee Claim",null,8]
["Non Conformity",null,2]
["Observation",null,3]
["Other",null,7]

{"sheet":"VIQrefno","index":6,"n_rows":1,"n_cols":3,"rows_kept":1,"cut":false,"hidden":true,"merged":[]}
["VIQ_ref_no","Risk Value of observation","ID"]

{"sheet":"Equipment_list","index":7,"n_rows":28,"n_cols":3,"rows_kept":28,"cut":false,"hidden":true,"merged":[]}
["TITLE","Equipment_list_description","ID"]
["Accommodation",null,12]
["Cargo Mach.",null,13]
["Critical Equip.",null,16]
["Deck - Machinery",null,18]
["Deck - Mooring Machinery",null,15]
["Deck - Pipe / Fittings",null,20]
["Documentation",null,21]
["E/R - Air Comp.",null,8]
["E/R - Aux. Engine",null,4]
["E/R - Aux. Mach.",null,7]
["E/R - Boiler",null,5]
["E/R - Main Engine",null,3]
["E/R - Pipes/ valves & fittings",null,9]
["E/R - Pumps",null,32]
["E/R - Purifier",null,6]
["Elect. Mach. & Equip.",null,10]
["Hull & Tanks",null,19]
["Inert Gas",null,14]
["LSA / FFA",null,17]
["Miscellaneous",null,22]
["Navigation - DGPS / EPFS / AIS",null,28]
["Navigation - ECDIS",null,25]
["Navigation - Echo Sounder / Speed Log",null,26]
["Navigation - GMDSS & Communication",null,23]
["Navigation - Others",null,11]
["Navigation - RADAR",null,24]
["Navigation - VDR / BNWAS",null,30]

{"sheet":"PSC_MOU","index":8,"n_rows":11,"n_cols":3,"rows_kept":11,"cut":false,"hidden":true,"merged":[]}
["TITLE","PSC_MOU_description","ID"]
["Asia and the Pacific",null,2]
["Caribbean",null,4]
["Europe and the North Atlantic",null,1]
["Latin America",null,3]
["The Black Sea region",null,6]
["The Indian Ocean",null,8]
["The Mediterranean",null,7]
["The Riyadh MoU",null,9]
["USCG",null,10]
["West and Central Africa",null,5]

{"sheet":"Inspection_type","index":9,"n_rows":13,"n_cols":2,"rows_kept":13,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Bunkering Audit",14]
["Cargo Audit",17]
["Engineering Audit",16]
["ISM Audit",2]
["ISPS Audit",3]
["IT Audit",10]
["MLC Audit",1]
["Mooring Audit",9]
["Nav Audit / Verification",8]
["Onboard Training",18]
["Ship Staff Insp.",15]
["Suptd. Insp.",13]

{"sheet":"Deficiency_Cause","index":10,"n_rows":8,"n_cols":3,"rows_kept":8,"cut":false,"hidden":true,"merged":[]}
["TITLE","Deficiency_Cause_description","ID"]
["Behaviour Based",null,1]
["Equipment Related",null,4]
["External Factors",null,5]
["Human Error",null,7]
["Inappropriate Procedure",null,8]
["Industry Issue",null,6]
["Knowledge Based",null,3]

{"sheet":"Observer_code","index":11,"n_rows":3,"n_cols":3,"rows_kept":3,"cut":false,"hidden":true,"merged":[]}
["TITLE","Observer_code_description","ID"]
["Owner / Marine / Tech. Suptd.",null,3]
["Ship Staff",null,2]

{"sheet":"Status_code","index":12,"n_rows":6,"n_cols":3,"rows_kept":6,"cut":false,"hidden":true,"merged":[]}
["TITLE","Status_code_description","ID"]
["Completed",null,6]
["Deferred to D D",null,5]
["In progress",null,3]
["Not Started",null,2]
["Waiting spare",null,4]

{"sheet":"PSC_ref_no","index":13,"n_rows":19,"n_cols":2,"rows_kept":19,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Alarms",9]
["Cargo operations including equipment",7]
["Certificates & Documentation",2]
["Dangerous Goods",13]
["Emergency Systems",5]
["Fire safety",8]
["ISM",16]
["ISPS",17]
["Life saving appliances",12]
["MLC, 2006",18]
["Other",19]
["Pollution Prevention",15]
["Propulsion and auxiliary machinery",14]
["Radio communication",6]
["Safety of Navigation",11]
["Structural condition",3]
["Water/Weathertight condition",4]
["Working and Living Conditions",10]

{"sheet":"Risk_value_of_obs","index":14,"n_rows":1,"n_cols":2,"rows_kept":1,"cut":false,"hidden":true,"merged":[]}
["Risk Value of observation","ID"]

{"sheet":"Year","index":15,"n_rows":18,"n_cols":1,"rows_kept":18,"cut":false,"hidden":true,"merged":[]}
["Year"]
[2014]
[2015]
[2016]
[2017]
[2018]
[2019]
[2020]
[2021]
[2022]
[2023]
[2024]
[2025]
[2026]
[2027]
[2028]
[2029]
[2030]

{"sheet":"Month","index":16,"n_rows":13,"n_cols":1,"rows_kept":13,"cut":false,"hidden":true,"merged":[]}
["Month"]
["Jan"]
["Feb"]
["Mar"]
["Apr"]
["May"]
["Jun"]
["Jul"]
["Aug"]
["Sep"]
["Oct"]
["Nov"]
["Dec"]

{"sheet":"Date_","index":17,"n_rows":32,"n_cols":1,"rows_kept":32,"cut":false,"hidden":true,"merged":[]}
["Date"]
["01"]
["02"]
["03"]
["04"]
["05"]
["06"]
["07"]
["08"]
["09"]
[10]
[11]
[12]
[13]
[14]
[15]
[16]
[17]
[18]
[19]
[20]
[21]
[22]
[23]
[24]
[25]
[26]
[27]
[28]
[29]
[30]
[31]

{"sheet":"Sheet1","index":18,"n_rows":24,"n_cols":6,"rows_kept":24,"cut":false,"hidden":true,"merged":[]}
[]
[null,"ID","E",null,"Date Recorded",1]
[null,"UNIQUE ID","F",null,"Type of Deficiency",2]
[1,"Date Recorded","G",null,"Observer code",3]
["ignore","Vessel Type","H",null,"Type of Inspection",4]
[null,"Internal / External","I",null,"Description of Deficiency",5]
[null,"Drydock","J",null,"Equipment Categories",6]
[null,"Information Sharing","K",null,"Area of Observation",7]
[null,"Critical_item","L",null,"Deficiency Cause",8]
[null,"Deficiency Type","M",null,"VIQ Ref Number",9]
[null,"Deficiency Cause","N",null,"Risk Value of Obs",10]
[null,"Inspection Type","O",null,"PSC Ref Number",11]
[null,"Equipments","P",null,"PSC MOU ID",12]
[null,"VIQ Reference Number","Q",null,"Action Taken or Required",13]
[null,"Risk Value of the observation","R",null,"Target Date",14]
[null,"PSC Reference Number","S",null,"PO Ref No.",15]
[null,"PSC MOU","T",null,"Status Code",16]
[null,"Observer Code","U",null,"Date Completed",17]
[null,"Target Date","V",null,"Drydock",18]
[null,"Status Code","W",null,"Info Sharing",19]
[null,"Description of Deficiency","X",null,"Critical Item Flag",20]
[null,"Action taken / required","Y",null,"Audit Type",21]
[null,"PO ref no","Z"]
[null,"Date completed","AA"]

{"sheet":"Ship_information","index":19,"n_rows":2,"n_cols":4,"rows_kept":2,"cut":false,"hidden":true,"merged":[]}
["Ship_ID","Ship_Name","FILE_NAME","Export_Date"]
["120","SUNRISE I (13-09-2023)","120_1694572884730.xlsm","2023-10-22 21:10:08"]

{"sheet":"External_Deficiency_type","index":20,"n_rows":5,"n_cols":3,"rows_kept":5,"cut":false,"hidden":true,"merged":[]}
["TITLE","Type of deficiency_description","ID"]
["Condn of Class / Memo",null,5]
["Defect",null,1]
["Non Conformity",null,2]
["Observation",null,3]

{"sheet":"External_Inspection_type","index":21,"n_rows":11,"n_cols":2,"rows_kept":11,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Cargo Audit",17]
["Flag State Insp.",5]
["ISM Audit",2]
["ISPS Audit",3]
["MLC Audit",1]
["Nav Audit / Verification",8]
["OM Insp. (Eg. SIRE / CDI etc.)",6]
["Others (Eg. Insurance etc.)",12]
["PSC Inspection",4]
["Terminal Insp.",11]

{"sheet":"External_Observer_code","index":22,"n_rows":7,"n_cols":3,"rows_kept":7,"cut":false,"hidden":true,"merged":[]}
["TITLE","Observer_code_description","ID"]
["Class Surveyor",null,4]
["FSC Inspector",null,5]
["Others (Eg. Insurance etc.)",null,9]
["PSC Insp.",null,6]
["SIRE / CDI Insp.",null,8]
["Terminal Insp.",null,7]

{"sheet":"Sheet Version","index":23,"n_rows":2,"n_cols":2,"rows_kept":2,"cut":false,"hidden":true,"merged":[]}
["Version","Title"]
["2.0","Version 2.0"]