{"text_format":"1","workbook":"xlsx","n_sheets":24,"sheets":["Mainsheet","Completed","Calc","Areaofobs","Vessel_type","Deficiency_type","VIQrefno","Equipment_list","PSC_MOU","Inspection_type","Deficiency_Cause","Observer_code","Status_code","PSC_ref_no","Risk_value_of_obs","Year","Month","Date_","Sheet1","Ship_information","External_Deficiency_type","External_Inspection_type","External_Observer_code","Sheet Version"],"not_rendered":{"charts":0,"images":1,"macros":1,"external_links":0,"defined_names":12,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Mainsheet","index":0,"n_rows":34,"n_cols":28,"rows_kept":34,"cut":false,"hidden":false,"merged":[[10,8,10,9],[10,12,10,13],[12,6,12,27],[8,6,8,27]]}
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,"Defect - Damage Monitoring Sheet"]
[]
[null,null,null,null,null,null,null,"Date of Report","01-Jan-2024",null,null,"Ship Name","DHT PUMA (24-08-2023)"]
[]
[null,null,null,null,null,null,"VERSION : 2.0"]
[]
[]
[]
[null,null,null,"ID","SHIPSIDE UNIQUEID","UNIQUE ID","Date Recorded","Type of Deficiency","Observer code","Type of Inspection","Description of Deficiency","Equipment Categories","Area of Observation","Deficiency Cause","VIQ Ref Number","Risk Value of Obs","PSC Ref Number","PSC MOU ID","Action Taken or Required","Target Date","PO Ref No.","Status Code","Date Completed","Drydock","Info Sharing","Critical Item","Audit Type","Superintendent Remarks"]
[null,null,null,null,13063,"0_Thu Feb 09 2023 16:44:58 GMT+0800","2023-01-29T08:00:00","Critical Equipment","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Port windlass anchor stopper spring broken.","Deck - Mooring Machinery","Mooring","Equipment Related","9.20","Medium","","","Port windlass stopper spring received at Singapore on 08-Dec-23. Waiting for suitable oppotunity to renew the spring.","2024-01-31T08:00:00","DPUM230023","In progress",null,"No","No","No","Internal","Noted on the RO for spare as per DPUM230023.\nWe will revert soonest on the RO."]
[null,null,null,30590,50485,"53_Sat Apr 22 2023 00:42:35 GMT+0800","2023-02-04T23:59:35","Defect","Ship Staff","Nav Audit / Verification","Bridge windows sunscreen (Shades) cleats and locks are damaged. Also, securing ropes condition is deteriorated","Navigation - Others,Miscellaneous","Navigation","Equipment Related","11.6","Medium","","","RO raised for spare parts and to be replaced once received.\nAwaiting stores to replace the defective ones.","2023-10-14T23:59:35","DPUM230064","Waiting spare",null,"No","No","No","Internal","The RO DPUM230064 raised is noted. Please use alternate means to sunscreen rope."]
[null,null,null,null,31581,"0_Wed Feb 22 2023 17:17:10 GMT+0800","2023-02-12T08:00:00","Observation","Ship Staff","Ship Staff Insp.","Aux. Boiler Dosing Pump found leaking by way of the seal","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","RO to be raised for spare pump & mechanical seals. DPUM230161, supply awaited Target date revised","2024-02-29T08:00:00","","Waiting spare",null,"No","No","No","Internal","Please advise RO Number for follow up."]
[null,null,null,null,98881,"0_Wed Feb 22 2023 17:34:51 GMT+0800","2023-02-12T08:00:00","Observation","Ship Staff","Ship Staff Insp.","Galley Oven 440V low insulation is detected from Heating element.","Elect. Mach. & Equip.","","Equipment Related","10.38","Medium","","","Presently oven heating element is isolated. \nRO DPUM230032 raised. Raised in January 23- supply awaited. Target date revised.","2024-01-31T08:00:00","DPUM230032","Waiting spare",null,"No","No","No","Internal","DPUM230032 - please confirm that the same is received and fitted."]
[null,null,null,null,86226,"0_Wed Feb 22 2023 17:36:29 GMT+0800","2023-02-12T08:00:00","Observation","Ship Staff","Ship Staff Insp.","Galley Hotplate 440V low insulation.","","General Appearance","Equipment Related","10.38","Medium","","","RO DPUM230032 raised.. Still awaiting supply. Target date amended due to long voyage.","2024-01-31T08:00:00","DPUM230032","Waiting spare",null,"No","No","No","Internal","Please confirm that RO has been received?"]
[null,null,null,null,48876,"0_Thu Feb 23 2023 17:52:19 GMT+0800","2023-02-12T08:00:00","Observation","Ship Staff","Ship Staff Insp.","BWTS electrolyzer flow meter FIT-1133 (Aft Peak) PCB is malfunctioning and currently it is kept in manual mode at constant flow.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","6.21","High","","","PCB is to be renewed. DPUM220153. This requires further investigation. Present state- awaiting maker go ahead for testing. Can only troubleshoot further. Target date revised owing to long voyage ahead.","2024-01-31T08:00:00","DPUM220153","Waiting spare",null,"No","No","No","Internal","Please send email on troubleshooting carried out. We will follow with Maker based on the vessel troubleshooting email. \nNoted on the RO DPUM220153 - but before we supply the DPUM220153, we need to be sure that this will solve the problem."]
[null,null,null,null,23968,"0_Thu Feb 23 2023 17:53:23 GMT+0800","2023-02-12T08:00:00","Observation","Ship Staff","Ship Staff Insp.","Aft Peak BWTS TRO unit sample inlet solenoid and pressure gauge is defective. ","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","6.21","High","","","RO DPUM230057 raised. System been tried out as per makers recommendations. Target date revised. ","2024-01-31T08:00:00","","Waiting spare",null,"No","No","No","Internal"]
[null,null,null,null,13934,"0_Thu Feb 23 2023 17:56:36 GMT+0800","2023-02-12T08:00:00","Observation","Ship Staff","Ship Staff Insp.","Electrolyzer unit C3, One power feeder PE coating is found damaged.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","6.21","High","","","Temporarily applied silicon to prevent water leakage.  RO raised for the same.\nDPUM230021. ( RO cancelled as per Tech.Manager advise. ) Vessel will raise separate RO for Flowmeter after discussion with Tech.Super.","2024-01-30T08:00:00","","In progress",null,"No","No","No","Internal",""]
[null,null,null,null,28186,"0_Thu Feb 23 2023 17:54:30 GMT+0800","2023-02-12T08:00:00","Observation","Ship Staff","Ship Staff Insp.","BWTS salinometer reading on local display is showing in percentage (0.36) instead of unit PSU. The operation log reports are showing value 5 PSU which is minimum acceptable 15 PSU.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","6.21","High","","","Shore guidance will be necessary for clarification and rectification. Target date revised. Will look into this and revert by next report.","2024-01-31T08:00:00","","Waiting spare",null,"No","No","No","Internal","Please send email on the trouble and trouble-shooting, we will seek maker guidance on how to sort out this issue."]
[null,null,null,null,16377,"53_Sun Apr 16 2023 03:47:25 GMT+0800","2023-03-29T08:00:00","Observation","Ship Staff","Ship Staff Insp.","AE #1 Pickup Sensor for Doctor Unit malfunctioning.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Pickup Sensor to be replaced. RO DPUM230051 raised. Awaiting supply. RO raised on 23rd January.  ","2024-01-31T08:00:00","DPUM230051","Waiting spare",null,"No","No","No","Internal","RO DPUM230051 for Pickup Sensor to be supplied soonest."]
[null,null,null,null,65226,"53_Mon May 15 2023 16:45:04 GMT+0800","2023-04-30T08:00:00","Observation","Ship Staff","Ship Staff Insp.","AE Viscotherm value showing 25cst at 130deg cent.","E/R - Aux. Engine,E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","The viscosity is showing 25cst at 130deg cent. Should show 13cst at 128 deg cent. When the sensor was removed, the viscosity showed 0 cst. On opening the bypass valve, the viscosity also shows 0 cst. Prior trouble, on LSMGO, the viscosity was showing 6cst at 36deg cent. Should have shown 4cst at 36deg cent. Shipstaff has opened up the sensor & cleaned the same. The locating pin also found missing & the hole oval. We have tried to reposition the sensor closest to the locating pin, however, there is no improvement. Suspect issue with the Sensor. RO \"DPUM230117\" raised. Awaiting spares. Spare awaited. At the moment showing correct reading for past 2 months. Under observation. ","2024-02-29T08:00:00","DPUM230117","Waiting spare",null,"No","No","No","Internal","Noted that the locating pin also found missing & the hole oval. Vessel has tried to reposition the sensor closest to the locating pin, however, there is no improvement. RO \"DPUM230117\" will be supplied to the vessel at First Opportunity."]
[null,null,null,null,36449,"0_Mon May 15 2023 19:32:12 GMT+0800","2023-05-06T08:00:00","Observation","Ship Staff","Ship Staff Insp.","EGCS Turbidity for WMS-001 showing higher value of more than 20.0FNU","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Turbidity sensor calibrated using the onboard calibration kit & procedure as per the manual. After calibration, the Inlet Turbidity still showing 18.8~21.2FNU. The sensor was re-calibrated again & stil no change in the Turbidity. GC raised for the same. Technician calibrated the sensor on 13-Jun-2023. Under observation. Showing high again.  Under observation now. ","2024-01-30T08:00:00","","In progress",null,"No","No","No","Internal","Noted that technician calibrated the sensor on 13-Jun-2023.  If the Turbidity sensor is ok under observation, the same can be closed."]
[null,null,null,null,27515,"0_Mon May 15 2023 19:36:26 GMT+0800","2023-05-06T08:00:00","Observation","Ship Staff","Ship Staff Insp.","EGCS WMS-002 Turbidity found reducing to 0.0FNU even after calibration.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Before Calibration Outlet Turbidity: 0.0FNU. Turbidity sensor calibrated using the onboard calibration kit & procedure as per the manual. After calibration, outlet Turbidity showing 4.0~5.0FNU. Turbidity reduced to 0.0FNU after a few hours of operation. GC raised for the same. Technician calibrated the sensor on 13-Jun-2023. Under observation. ","2024-01-31T08:00:00","","In progress",null,"No","No","No","Internal","Noted that technician calibrated the sensor on 13-Jun-2023. If the Turbidity sensor is ok under observation, the same can be closed."]
[null,null,null,30603,57404,"53_Mon Jun 05 2023 09:27:45 GMT+0800","2023-05-15T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Medical oxygen bottle Regulator need to be serviced or replaced every 5 years as per maker's instructions.\nAlso, Service enginer, who attended the vessel at Singpore on 25 Jan 2023, advised to replace the regulators.","Miscellaneous","Safety / LSA / FFA","Equipment Related","5.4","High","","","RO RAISED, AWAITING SPARE","2023-09-29T23:59:35","DPUM230059","Waiting spare",null,"No","No","No","Internal","Noted on same- the Medical oxygen bottle Regulator available ex-stock is not suitable for ship use. we will check further and update"]
[null,null,null,null,48857,"53_Wed Jun 14 2023 09:11:08 GMT+0800","2023-06-07T08:00:00","Observation","Ship Staff","Ship Staff Insp.","ME LO Pump #1 Starter Panel short circuit","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Short circuit caused the following:\n1.\tNo.1 ME LO Pump breaker damaged– All busbar linkages have been removed. The main breaker & base has been removed.\n2.\tNo.1 Stern Tube LO Pump Starter panel – All busbar linkages have been removed.\n3.\tNo.1 ME Jacket Cooling FW Pump Starter panel – All busbar linkages have been removed.\n4.\tNo .1 Composite Boiler Feed Water Pump - All busbar linkages have been removed. Same under investigation.\n\nReceived spares and job in hand.\nRequested workshop help to complete this job while vessel bunkers in SIngapore. Should not be done while sailing. Vessel is doing long voyages. In ports ETO occupied with BWTS attention as equipment requires constant attention. In ports cargo loading discharging PSC/ Oil major inspections etc. Starter panels complete replaced by shore contractor with constant assistance from our ETO. Running for past one week and seems okay. Will update once confirmed running okay for a month as per email from Mr. Kamlesh Solanki. Will close , if all okay, next fortnight.","2024-01-30T08:00:00","","In progress",null,"No","No","No","Internal","Hyundai Service Engineer from Korea will attend the vessel at Singapore anchorage for the root cause of this damage. Mr. Sajeesh is following on permanent repair. we will revert with details when the all the spares are ready for this rectification."]
[null,null,null,null,74510,"53_Tue Oct 31 2023 17:42:11 GMT+0800","2023-10-23T08:00:00","Breakdown","Ship Staff","Ship Staff Insp.","4S Water Ballast Tank sounding gauge in CCR is in-opeartional and showing in-correct sounding of tanks. ","Cargo Mach.","Cargo / Ballast Systems","Equipment Related,Inappropriate Procedure","8.8","Medium","","","Sounding gauge pneumatic indication unit is not damaged. Vessel raised RO DPUM230234: ELECTRO PNEUMATIC TYPE TANK  LEVEL & DRAFT GUAGING SYSTEM","2023-12-30T08:00:00","DPUM230234: ELECTRO PNEUMATIC TYPE TANK  LEVEL & DRAFT GUAGING SYSTEM","Waiting spare",null,"No","No","No","Internal"]
[null,null,null,null,40362,"53_Sun Dec 17 2023 22:29:21 GMT+0800","2023-12-08T08:00:00","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Paint MSDS to be checked if latest (onboard MSDS is issued in 2014)","Documentation","Safety / LSA / FFA","Inappropriate Procedure","5.46","Medium","","","latest paint MSDS to be downloaded and posted in paint locker.","2024-01-08T08:00:00","","Not Started",null,"No","No","No","Internal"]

{"sheet":"Completed","index":1,"n_rows":644,"n_cols":28,"rows_kept":644,"cut":false,"hidden":false,"merged":[[10,8,10,9],[10,12,10,13],[12,6,12,27],[8,6,8,27]]}
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,"Defect - Damage Monitoring Sheet"]
[]
[null,null,null,null,null,null,null,"Date of Report","01-Jan-2024",null,null,"Ship Name","DHT PUMA (24-08-2023)"]
[]
[null,null,null,null,null,null,"VERSION : 2.0"]
[]
[]
[]
[null,null,null,"ID","SHIPSIDE UNIQUEID","UNIQUE ID","Date Recorded","Type of Deficiency","Observer code","Type of Inspection","Description of Deficiency","Equipment Categories","Area of Observation","Deficiency Cause","VIQ Ref Number","Risk Value of Obs","PSC Ref Number","PSC MOU ID","Action Taken or Required","Target Date","PO Ref No.","Status Code","Date Completed","Drydock","Info Sharing","Critical Item","Audit Type","Superintendent Remarks"]
[null,null,null,715,null,"53_14/10/2019 10:25:44 AM","2018-06-16T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Item 6 (02/2018): Mechanical damage of paint observed on stbd side on top side between no.1 and no.2 WBT. Small rust patches are also visible in way of cargo manifold- port side","Hull & Tanks","General Appearance","External Factors","","","","","Starboard side Completed. Port Side completed at Juaymah anchorage.","2019-05-23T23:59:35","","Completed","2019-07-27T23:59:35","No","No","No","Internal"]
[null,null,null,9465,null,"53_08/01/2020 4:10:40 PM","2019-01-06T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Lifeboats 3 monthly drills were carried out at Angra Dos Reis Anchorage . While picking up the lifeboat the limit switch for the manual lifting of the wire drum was found in operational.","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.28","Very High","","","Limit switch repaired and checked for correct operation","2019-01-06T23:59:35","","Completed","2019-01-06T23:59:35","No","No","No","Internal"]
[null,null,null,9466,null,"53_08/01/2020 4:19:46 PM","2019-02-21T23:59:35","Non Conformity","Ship Staff","Ship Staff Insp.","Old Isolation permit was used.","Documentation","Cert. & Docu.","Human Error,Knowledge Based","5.2","Very High","","","Old form was discarded.A copy of fleet memo was displayed at workstations till the new checklist was reflected in the QDMS.","2019-02-21T23:59:35","","Completed","2019-02-21T23:59:35","No","No","No","Internal"]
[null,null,null,10214,null,"53_29/01/2020 3:52:29 PM","2019-02-26T23:59:35","Non Conformity","PSC Insp.","PSC Inspection","No Evidence available that emergency lighting for muster and embarkation station tested during abandonship drill","LSA / FFA","Safety / LSA / FFA","Knowledge Based","","","Life saving appliances","","Concerned officer's briefed about same and further drill reports corrected accordingly","2019-02-26T23:59:35","","Completed","2019-02-26T23:59:35","No","No","No","External"]
[null,null,null,10215,null,"53_29/01/2020 4:13:37 PM","2019-02-26T23:59:35","Non Conformity","PSC Insp.","PSC Inspection","Training record for ballast water management manual not available in BWMP","Miscellaneous","Cargo / Ballast Systems","Knowledge Based","","","Other","","Records were maintained in separate file for all trainings conducted. However, inspectors emphasised to have these records to be updated in Ballast Water Management Manual.\n\n\n\n","2019-02-26T23:59:35","","Completed","2019-02-26T23:59:35","No","No","No","External"]
[null,null,null,9463,null,"53_08/01/2020 3:55:36 PM","2019-02-27T23:59:35","Non Conformity","Owner / Marine / Tech. Suptd.","Nav Audit / Verification","Security chart was not readily available as it was stowed with other charts","Navigation - Others","Navigation","Human Error,Knowledge Based","7.13","Medium","","","Officers were briefed,matter to be discussed in passage plan meeting every time.","2019-03-24T23:59:35","","Completed","2019-03-08T23:59:35","No","No","No","Internal"]
[null,null,null,9464,null,"53_08/01/2020 4:02:05 PM","2019-02-27T23:59:35","Non Conformity","Owner / Marine / Tech. Suptd.","Nav Audit / Verification","Evidence of cross bearings & Transit bearings not available","Navigation - ECDIS","Navigation","Behaviour Based,Human Error,Knowledge Based","4.2","Medium","","","All officers were briefed,To be discussed in passage plan meeting","2019-03-24T23:59:35","","Completed","2019-03-08T23:59:35","No","No","No","Internal"]
[null,null,null,680,null,"53_13/10/2019 7:53:02 PM","2019-03-14T23:59:35","Critical Equipment","Ship Staff","Ship Staff Insp.","ODME not operational, Oil content meter failure","Critical Equip.","Cargo / Ballast Systems","Equipment Related","","","","","Halogen lamp to be replaced","2019-04-03T23:59:35","DPUM190006","Completed","2019-03-24T23:59:35","No","No","No","Internal"]
[null,null,null,684,null,"53_13/10/2019 8:50:49 PM","2019-03-27T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Service Air Compressor motor winding insulation got burned and insulation resistance become zero because of one of the welded contact in main contactor and burning marks was found in OCR unit and MSB Circuit Breaker","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related","","","","","Newly received electric motor fitted and damaged contactor replaced / repaired  and service air compressor put back into service","2019-04-18T23:59:35","","Completed","2019-04-27T23:59:35","No","No","No","Internal"]
[null,null,null,681,null,"53_13/10/2019 8:19:46 PM","2019-04-18T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","(Item 3) L-8 panel, earth fault meter not functional","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","Ear fault meter inspected and found source power not available due to damage fuse, same replaced","2019-04-18T23:59:35","","Completed","2019-04-26T23:59:35","No","No","No","Internal"]
[null,null,null,682,null,"53_13/10/2019 8:30:54 PM","2019-04-18T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","(Item 6) COP #2 discharge valve controller malfunction","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","Valve inspected and found the positioner damaged. Positioner renewed and discharge valve operation","2019-05-03T23:59:35","","Completed","2019-04-29T23:59:35","No","No","No","Internal"]
[null,null,null,683,null,"53_13/10/2019 8:37:25 PM","2019-04-18T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","(Item 9) Ship specific UMS check list","Documentation","Cert. & Docu.","Human Error","","","","","Ship specific UMS checklist prepared and put in use","2019-06-18T23:59:35","","Completed","2019-04-29T23:59:35","No","No","No","Internal"]
[null,null,null,685,null,"53_13/10/2019 8:57:07 PM","2019-04-18T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","(Item 17) STBD boiler blow down line vibrating near the port / fwd feet of the boiler","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","Clamping arrangement fabricated and fitted to restrict the vibration of blow down line.","2019-05-18T23:59:35","","Completed","2019-05-01T23:59:35","No","No","No","Internal"]
[null,null,null,686,null,"53_13/10/2019 9:58:05 PM","2019-04-18T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","(Item 11) Accom AC #1 compressor belts fluttering","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Belt tencion adjusted as required to prevent the fluttering of belts","2019-05-03T23:59:35","","Completed","2019-05-01T23:59:35","No","No","No","Internal"]
[null,null,null,687,null,"53_13/10/2019 10:18:26 PM","2019-04-18T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Minute hydraulic leaks from STBD windlass break operation piston side and isolation valve","Deck - Mooring Machinery","Mooring","Equipment Related","","","","","Flange tightened and leaks arrested.","2019-04-28T23:59:35","","Completed","2019-05-03T23:59:35","No","No","No","Internal"]
[null,null,null,688,null,"53_13/10/2019 10:23:31 PM","2019-04-18T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Entrance area need to be cleaned and the deck head painted","Hull & Tanks","General Appearance","Equipment Related","","","","","cleaned and painted","2019-04-26T23:59:35","","Completed","2019-05-02T23:59:35","No","No","No","Internal"]
[null,null,null,689,null,"53_13/10/2019 10:29:03 PM","2019-04-18T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","(Item 18) Smoke room bulkheads to scrub off yellow deposits ","Miscellaneous","General Appearance","Behaviour Based","","","","","Cleaning carried out.","2019-04-28T23:59:35","","Completed","2019-05-01T23:59:35","No","No","No","Internal"]
[null,null,null,690,null,"53_13/10/2019 10:34:45 PM","2019-04-18T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","(Item 4) Resting post is vibrating while sailing. The stay wires apparently appear to be loose.","Miscellaneous","Structural Condn. / WT integrity ","External Factors","","","","","Stay Wire Tightned","2019-05-03T23:59:35","","Completed","2019-04-28T23:59:35","No","No","No","Internal"]
[null,null,null,691,null,"53_13/10/2019 10:39:20 PM","2019-04-18T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","(Item 15) ODME procedures and line diagram not posted in pump room","Cargo Mach.","Cargo / Ballast Systems","Inappropriate Procedure","","","","","Procedure pasted","2019-04-28T23:59:35","","Completed","2019-05-20T23:59:35","No","No","No","Internal"]
[null,null,null,692,null,"53_13/10/2019 10:43:33 PM","2019-04-18T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","(Item 16) Sign of water ingress in Stbd Lifeboat","LSA / FFA","Safety / LSA / FFA","External Factors","","","","","cleaned","2019-04-28T23:59:35","","Completed","2019-04-27T23:59:35","No","No","No","Internal"]
[null,null,null,694,null,"53_13/10/2019 10:54:35 PM","2019-04-18T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","(Item 8) AHU fresh air intake grid to derust and polish","Miscellaneous","General Appearance","Behaviour Based,External Factors","","","","","Derusting and polishing to be carrried out","2019-05-03T23:59:35","","Completed","2019-05-02T23:59:35","No","No","No","Internal"]
[null,null,null,695,null,"53_13/10/2019 11:04:47 PM","2019-04-18T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","(Item 13) Pump room guide wire to be secure to the top coming. to unable to open the hatch without the need to unsecure from bottom connection.","Miscellaneous","General Appearance","Inappropriate Procedure","","","","","Wire  secured to top platform","2019-06-18T23:59:35","","Completed","2019-05-19T23:59:35","No","No","No","Internal"]
[null,null,null,696,null,"53_14/10/2019 5:49:39 PM","2019-04-18T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","(Item 14) WB stripping Educator suction gauge showing faulty reading and vibrating.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","Fault rectified","2019-06-18T23:59:35","","Completed","2019-05-03T23:59:35","No","No","No","Internal"]
[null,null,null,697,null,"53_14/10/2019 6:21:27 PM","2019-04-18T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","(item 5) Manifold reducers stowing tray to be made in the midship stores and shift the reducers in the midship store","Miscellaneous","General Appearance","Inappropriate Procedure","","","","","reducers  shifted to midship store.","2019-05-18T23:59:35","","Completed","2019-05-18T23:59:35","No","No","No","Internal"]
[null,null,null,700,null,"53_14/10/2019 4:34:30 AM","2019-04-18T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","(Item 1) Pump Room natural vent mushroom, Wire mesh support frame rivets are broken.","Miscellaneous","General Appearance","Equipment Related","","","","","Wire Mesh to riveted back.","2019-06-18T23:59:35","","Completed","2019-05-31T23:59:35","No","No","No","Internal"]
[null,null,null,701,null,"53_14/10/2019 4:37:38 AM","2019-04-18T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","(item 2) There is lot of gap between the weight and the pin while chain in pace. Sleeve to fabricate.","Miscellaneous","General Appearance","Inappropriate Procedure","","","","","Sleeve to be fabricated","2019-06-18T23:59:35","","Completed","2019-06-03T23:59:35","No","No","No","Internal"]
[null,null,null,702,null,"53_14/10/2019 4:41:30 AM","2019-04-18T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","(Item 12) Side cushy mounting damaged, to renew","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Service air Compressor side cushy mountings received and replaced the damaged ones.","2019-06-18T23:59:35","DPUM190078","Completed","2019-07-09T23:59:35","No","No","No","Internal"]
[null,null,null,703,null,"53_14/10/2019 4:45:13 AM","2019-04-18T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","(Item 7) Paint crack on the main deck weld seams, the primer coat still intact,","Hull & Tanks","General Appearance","External Factors","","","","","Buffing and painting completed","2019-06-18T23:59:35","","Completed","2019-06-28T23:59:35","No","No","No","Internal"]
[null,null,null,717,null,"53_14/10/2019 10:31:15 AM","2019-04-18T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","(Item 10) Boiler local control panel to fit with AC /cooling unit","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","Transferred to REFMAN drydock defect monitoring","2019-06-18T23:59:35","","Completed","2019-08-29T23:59:35","No","No","No","Internal"]
[null,null,null,693,null,"53_13/10/2019 10:48:16 PM","2019-05-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Ship performance monitoring system display unit KDU 200 defective and not giving the power and torque paramaters","Miscellaneous","Cargo / Ballast Systems","Equipment Related","","","","","Replaced with uupdated KDU 210 and working normal","2019-06-23T23:59:35","","Completed","2019-05-23T23:59:35","No","No","No","Internal"]
[null,null,null,698,null,"53_14/10/2019 6:25:21 PM","2019-05-25T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Fresh water generator ejector pump suction line sacrificail flange leakage","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Sacrificial flange replaced with new one and leakage rectified","2019-06-03T23:59:35","","Completed","2019-05-28T23:59:35","No","No","No","Internal"]
[null,null,null,699,null,"53_14/10/2019 4:30:39 AM","2019-05-25T23:59:35","Defect","Ship Staff","Ship Staff Insp.","LSFO bunker tank level guage reading showing zero even though tank is full","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Trouble shoot carried out and found the pneumatic modular unit for the tank was defective and replaced with spare one","2019-06-23T23:59:35","","Completed","2019-05-28T23:59:35","No","No","No","Internal"]
[null,null,null,9467,null,"53_08/01/2020 4:24:15 PM","2019-06-24T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Citadel does not have satellite phone connection. The previous sim card for satellite phone was discontinued due to change if system to Speed cast.","Critical Equip.","Safety / LSA / FFA","Equipment Related","7.6","Medium","","","It is not mandatory to have satellite phone in Citadel.","2019-07-01T23:59:35","","Completed","2019-06-28T23:59:35","No","No","No","Internal"]
[null,null,null,704,null,"53_14/10/2019 4:48:23 AM","2019-07-04T23:59:35","Defect","Ship Staff","Ship Staff Insp.","COW Root v/v of 3W(Aft) hard to open/close & not holding","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","","","","","Overhauling of Root v/v carried out, Gear box inspected and greased.","2019-07-18T23:59:35","","Completed","2019-07-06T23:59:35","No","No","No","Internal"]
[null,null,null,705,null,"53_14/10/2019 4:51:14 AM","2019-07-08T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Drain v/v OD328 to 4S COT at Manifold hard to operate","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","","","","","Inspection and Greasing of gearbox carried out.","2019-07-18T23:59:35","","Completed","2019-07-09T23:59:35","No","No","No","Internal"]
[null,null,null,706,null,"53_14/10/2019 9:20:29 AM","2019-07-08T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Marpol v/v OD315 s/s Line 1 hard to open/shut","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","","","","","Inspection and Greasing of gearbox carried out.","2019-07-18T23:59:35","","Completed","2019-07-09T23:59:35","No","No","No","Internal"]
[null,null,null,707,null,"53_14/10/2019 9:23:46 AM","2019-07-08T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Manifold crossover v/v OD307 hard to operate","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","","","","","Overhauling and Greasing of v/v carried out.","2019-07-18T23:59:35","","Completed","2019-07-17T23:59:35","No","No","No","Internal"]
[null,null,null,708,null,"53_14/10/2019 9:27:38 AM","2019-07-08T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Marpol v/v OD316 s/s Line 1 hard to open/shut","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","","","","","Inspection and Greasing of gearbox carried out.","2019-07-18T23:59:35","","Completed","2019-07-17T23:59:35","No","No","No","Internal"]
[null,null,null,709,null,"53_14/10/2019 9:30:56 AM","2019-07-16T23:59:35","Defect","Ship Staff","Ship Staff Insp.","COW Root v/v of 2W(Aft) & 2C no.5 hard to open/close","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","","","","","Overhauling of Root v/v carried out, Gear box inspected and greased.","2019-07-18T23:59:35","","Completed","2019-07-18T23:59:35","No","No","No","Internal"]
[null,null,null,710,null,"53_14/10/2019 9:34:05 AM","2019-07-16T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Marpol v/v no.1 portside OD 317 and Goose neck v/v  OD301 hard to operate.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","","","","","Ispection and greasing of gearbox carried out, both v/v's easy to operate.","2019-07-22T23:59:35","","Completed","2019-07-19T23:59:35","No","No","No","Internal"]
[null,null,null,711,null,"53_14/10/2019 9:37:01 AM","2019-07-20T23:59:35","Defect","Ship Staff","Ship Staff Insp.","3S IG branch valve hard to operate","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","","","","","Inspection and Greasing of gearbox carried out.","2019-07-24T23:59:35","","Completed","2019-07-24T23:59:35","No","No","No","Internal"]
[null,null,null,712,null,"53_14/10/2019 9:39:26 AM","2019-07-25T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Main engine unit 7 HCU unit have leakage of oil from the accumulator flange","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Unit 7 accumulator flange removed and sealing ring 053 renewed, leakage continued. Removed the accumulator flange and the end plug removed and bonded seal rings renewed","2019-09-23T23:59:35","","Completed","2019-07-26T23:59:35","No","No","No","Internal"]
[null,null,null,713,null,"53_14/10/2019 9:41:42 AM","2019-07-25T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Leakage from the sacrificial anode flange of the LT cooler 1 sea water inlet line","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Sacrifical anode renewed","2019-08-23T23:59:35","","Completed","2019-07-27T23:59:35","No","No","No","Internal"]
[null,null,null,714,null,"53_14/10/2019 9:43:53 AM","2019-07-25T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Leakage from the sacrificial anode flange of the LT cooler 2 sea water inlet line","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Sacrifical anode renewed","2019-08-23T23:59:35","","Completed","2019-07-28T23:59:35","No","No","No","Internal"]
[null,null,null,716,null,"53_14/10/2019 10:28:49 AM","2019-07-30T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Observed pin hole leak from ballast line between BWTS filter and BA 40.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","Distance piece from the line removed and transferred to E/R workshop, Welding carried out and fitted back, pressure tested no leak observed.","2019-08-24T23:59:35","","Completed","2019-08-06T23:59:35","No","No","No","Internal"]
[null,null,null,718,null,"53_14/10/2019 10:34:10 AM","2019-08-26T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Minor leakage of lubricating oil from the inlet line flange to the exhuast valve actuator","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","System isolated and leakage from the flange to the actuator rectified","2019-09-04T23:59:35","","Completed","2019-09-04T23:59:35","No","No","No","Internal"]
[null,null,null,9468,null,"53_08/01/2020 4:31:05 PM","2019-09-07T23:59:35","Non Conformity","Ship Staff","Ship Staff Insp.","During discharge operations vessel had issued a pump room entry permit on 14th Sept 2019 valid from 0050 to 0800 hrs lt.\n\nHowever ETO & Chief Engineers had entered in pumproom at 0850 hrs lt is after the expiry of permit.","Documentation","ISM Related","Human Error,Knowledge Based","5.2","Very High","","","Immediately pumproom permit was verified and new permit was issued, Briefed the OOW to recheck Permit validity during taking over watch.","2019-09-07T23:59:35","","Completed","2019-09-07T23:59:35","No","No","No","Internal"]
[null,null,null,719,null,"53_14/10/2019 10:36:32 AM","2019-09-09T23:59:35","Defect","Ship Staff","Ship Staff Insp.","4S IG BRANCH VALVE HARD TO OPERATE","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","","","","","O/H AND GREASING OF GEAR BOX CARRIED OUT","2019-09-23T23:59:35","","Completed","2019-09-11T23:59:35","No","No","No","Internal"]
[null,null,null,720,null,"53_14/10/2019 10:38:39 AM","2019-09-09T23:59:35","Defect","Ship Staff","Ship Staff Insp.","4C IG BRANCH VALVE HARD TO OPERATE","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","","","","","O/H AND GREASING OF GEAR BOX CARRIED OUT","2019-09-23T23:59:35","","Completed","2019-09-12T23:59:35","No","No","No","Internal"]
[null,null,null,678,null,"53_13/10/2019 7:58:02 PM","2019-09-14T23:59:35","Defect","Ship Staff","Ship Staff Insp.","BWTS discharge rate measuring flow meter defective","Elect. Mach. & Equip.","Cargo / Ballast Systems","Equipment Related","8.8","Medium","","","renewed with the new spares recieved","2020-06-10T23:59:35","","Completed","2020-06-15T23:59:35","No","No","No","Internal","as per telcon on 30th Jan , it is notified system fault rectified. issue with the soln valves. kindly close out and update the list\nspare cartridgr RO was put in place"]
[null,null,null,627,null,"53_Invalid date","2019-09-24T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Drain valve of vapour line stbdside fwd, lower side found not holding.","Elect. Mach. & Equip.","Cargo / Ballast Systems","Equipment Related","","","","","Overhauling of the valve done, tested and fitted back.","2019-09-28T23:59:35","","Completed","2019-09-26T23:59:35","No","No","No","Internal"]
[null,null,null,679,null,"53_15/10/2019 4:51:49 AM","2019-09-24T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Flow Fault alarm was getting activated for ballast tank gas sampling system.","Elect. Mach. & Equip.","Cargo / Ballast Systems","Equipment Related","5.21","Medium","","","Checked pressure switch(PS1) found rubber membrane damage, temporary repairs were carried out, Requisition for the Spare raised. Ballast Tank Gas Detection system presently working satisfactory.","2019-12-08T23:59:35","DPUM190146","Completed","2019-12-19T23:59:35","No","No","No","Internal","to replace on receipt of spares, spares processed -follow with procure"]
[null,null,null,6734,null,"53_Fri Jan 11 2019 20:37:41 GMT+0000 (Coordinated Universal Time)","2019-10-08T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Moderate Rust observed at the 1S/2S shipside onthe stbdside.","Hull & Tanks","General Appearance","External Factors","11.2","Medium","","","De-rusting / Painting carried out, Santos Anchorage Brazil.","2019-12-24T23:59:35","","Completed","2019-10-30T23:59:35","No","No","No","Internal"]
[null,null,null,8757,null,"53_23/12/2019 20:39:42","2019-10-09T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Minor weeping marks from  sea water inlet line of LT Cooler 1","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Sea water inlet line sacrificial flange and gasktes renewed","2019-11-19T23:59:35","","Completed","2019-10-18T23:59:35","No","No","No","Internal"]
[null,null,null,6733,null,"53_Fri Jan 11 2019 13:35:01 GMT+0000 (Coordinated Universal Time)","2019-10-09T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Composite boiler fuel oil inlet line electric trace heater not working","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Requisition No. DPUM190190 raised, Defective Electric trace heater to be renewed after receiving the spare","2019-10-18T23:59:35","DPUM190190","Completed","2019-12-19T23:59:35","No","No","No","Internal","Spares arrangement in process, to followup with Purchase"]
[null,null,null,8758,null,"53_23/12/2019 20:44:02","2019-10-10T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Minor leakage of lub oil from ME Unit 3 exhaust valve actuator","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","ME Unit 3 exhaust valve actuator lub oil inlet line flange gasket renewed and union retightened","2019-10-17T23:59:35","","Completed","2019-10-15T23:59:35","No","No","No","Internal"]
[null,null,null,8759,null,"53_23/12/2019 20:28:22","2019-10-10T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ME Unit 7 minor lub oil leakage from accumulator flange","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","ME Unit accumulator flange sealing ring renwed","2019-10-17T23:59:35","","Completed","2019-10-15T23:59:35","No","No","No","Internal"]
[null,null,null,721,null,"53_14/10/2019 10:40:38 AM","2019-10-13T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","4P IG BRANCH VALVE HARD TO OPERATE","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.23","Medium","","","O/H AND GREASING OF GEAR BOX CARRIED OUT","2019-10-23T23:59:35","","Completed","2019-10-14T23:59:35","No","No","No","Internal"]
[null,null,null,722,null,"53_14/10/2019 10:42:50 AM","2019-10-13T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Slop-S, 5S, 5C IG BRANCH VALVE HARD TO OPERATE","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.23","Medium","","","O/H AND GREASING OF GEAR BOX CARRIED OUT","2019-10-23T23:59:35","","Completed","2019-10-22T23:59:35","No","No","No","Internal"]
[null,null,null,723,null,"53_14/10/2019 10:44:45 AM","2019-10-13T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","5P IG BRANCH VALVE HARD TO OPERATE","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.23","Medium","","","O/H AND GREASING OF GEAR BOX CARRIED OUT","2019-10-23T23:59:35","","Completed","2019-10-18T23:59:35","No","No","No","Internal"]
[null,null,null,724,null,"53_14/10/2019 10:52:49 AM","2019-10-13T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","COP#2 DRAIN VALVE SUSPECTED NOT HOLDING","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.11","Medium","","","RISER LINE DRAIN V/V OVERHAULED AND FITTED BACK.","2019-10-23T23:59:35","","Completed","2019-10-17T23:59:35","No","No","No","Internal"]
[null,null,null,725,null,"53_14/10/2019 11:29:54 AM","2019-10-13T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","CARGO EDUCTOR GAUGES SHOWING ERRATIC READING","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.12","Medium","","","CALIBRATION OF ALL CARGO EDUCTOR GAUGES CARRIED OUT.","2019-10-23T23:59:35","","Completed","2019-10-19T23:59:35","No","No","No","Internal"]
[null,null,null,726,null,"53_14/10/2019 11:31:42 AM","2019-10-13T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","SLOP-P BRANCH VALVE HARD TO OPERATE","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.23","Medium","","","O/H AND GREASING OF GEARBOX CARRIED OUT","2019-10-13T23:59:35","","Completed","2019-10-13T23:59:35","No","No","No","Internal"]
[null,null,null,9462,null,"53_08/01/2020 1:27:05 PM","2019-10-15T23:59:35","Non Conformity","Ship Staff","Ship Staff Insp.","Sea water leacage from sea water outlet sacrificial flange of low temp.cooler No:2.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Sacrificial flange of low temp.cooler No:2 was renew by spare.","2019-10-22T23:59:35","","Completed","2019-10-18T23:59:35","No","No","No","Internal"]
[null,null,null,6730,null,"53_Fri Nov 01 2019 18:04:38 GMT+0000 (Coordinated Universal Time)","2019-10-18T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Moderate Rust observed on the Main Mast","Critical Equip.,Deck - Pipe / Fittings,Miscellaneous","General Appearance","External Factors","11.8","Low","","","De-rusting and painting of Main mast carried out.","2019-10-24T23:59:35","","Completed","2019-10-23T23:59:35","No","No","No","Internal"]
[null,null,null,6731,null,"53_Fri Nov 01 2019 19:01:50 GMT+0000 (Coordinated Universal Time)","2019-10-18T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Stern of the shipside Moderate rust observed, need to be derusted and painted at anchorage.","Hull & Tanks","General Appearance","External Factors","11.1","High","","","Spot chipping/Painting carried out.","2019-10-24T23:59:35","","Completed","2019-10-19T23:59:35","No","No","No","Internal"]
[null,null,null,6732,null,"53_Fri Jan 11 2019 20:48:24 GMT+0000 (Coordinated Universal Time)","2019-10-18T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Manifold drip tray drain line to the valve found clogged.","Deck - Pipe / Fittings","Cargo / Ballast Systems","External Factors","6.6","Medium","","","Opened the section of pipe and cleared all rust/paint particles.","2019-10-24T23:59:35","","Completed","2019-10-23T23:59:35","No","No","No","Internal"]
[null,null,null,727,null,"53_15/10/2019 4:55:34 AM","2019-10-18T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Drain valve of vapour line stbdside fwd, lower side found not holding.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.19","High","","","Overhauling of the valve done, tested and fitted back.","2019-10-23T23:59:35","","Completed","2019-10-21T23:59:35","No","No","No","Internal"]
[null,null,null,9461,null,"53_08/01/2020 1:15:13 PM","2019-11-09T23:59:35","Non Conformity","Ship Staff","Ship Staff Insp.","Engine room blower flaps No:3 not closed.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Human Error","10.32","Very High","","","Flaps local operating control valve filter was clean from paint.","2019-11-10T23:59:35","","Completed","2019-11-09T23:59:35","No","No","No","Internal"]
[null,null,null,7992,null,"53_Fri Dec 06 2019 21:02:52 GMT+0000 (Coordinated Universal Time)","2019-11-18T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Inspection of COW Lines Expansion Joint.","Deck - Pipe / Fittings","Cargo / Ballast Systems","External Factors","8.34","High","","","During routine inspection of COW Lines Expansion Joint near 2C, 3C, 4C NBR rubber packing was found damage, same renewed, greased and boxed back. ","2019-11-24T23:59:35","DPUM190214","Completed","2019-11-22T23:59:35","No","No","No","Internal"]
[null,null,null,7993,null,"53_Wed Jun 12 2019 21:10:41 GMT+0000 (Coordinated Universal Time)","2019-11-21T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Fire Line Lines Expansion Joint found leaking.","Deck - Pipe / Fittings","Safety / LSA / FFA","External Factors","5.38","High","","","Fire Lines Expansion Joint near 3C rubber packing was found damage, same renewed, greased and boxed back.","2019-11-24T23:59:35","","Completed","2019-11-23T23:59:35","No","No","No","Internal"]
[null,null,null,9469,null,"53_08/01/2020 5:01:19 PM","2019-12-22T23:59:35","Non Conformity","Ship Staff","Ship Staff Insp.","During pre arrival port checks it was found that flow control valve for fixed Sopep wilden pump was closed rendering the pump unusable in case of emergency.","Deck - Machinery","MARPOL Related","Human Error","6.3","Low","","","Flow control valve was opened and readiness of pump checked,found in good working order.","2019-12-23T23:59:35","","Completed","2019-12-23T23:59:35","No","No","No","Internal"]
[null,null,null,10613,null,"53_28/02/2020 6:45:27 AM","2019-12-25T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Mooring winches M9 & M10 found with thick rusts in few places.","Deck - Mooring Machinery","Mooring","Equipment Related,Inappropriate Procedure","","","","","Derusting and painting of Mooring winches completed","2020-02-27T23:59:35","","Completed","2020-02-27T23:59:35","No","No","No","Internal"]
[null,null,null,10216,null,"53_29/01/2020 11:20:26 AM","2020-01-12T23:59:35","Critical Equipment","Ship Staff","Ship Staff Insp.","Fixed gas detetction system for Pumproom giving flow fault alarm for exhaust trunk sample points.","Critical Equip.","Safety / LSA / FFA","Equipment Related","5.22","High","","","P & S side Exhaust trunks opened,filters cleaned.System restarted,No alarms in system. ","2020-01-15T23:59:35","","Completed","2020-01-13T23:59:35","No","No","No","Internal"]
[null,null,null,10217,null,"53_29/01/2020 10:59:55 AM","2020-01-15T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Valve from VECS line at manifold to main I.G line found seized.","Inert Gas","Cargo / Ballast Systems","Equipment Related","8.17","Low","","","Gear box for the valve opened,Lubrication done,grease renewed. ","2020-01-16T23:59:35","","Completed","2020-01-16T23:59:35","No","No","No","Internal"]
[null,null,null,10614,null,"53_28/02/2020 6:49:27 AM","2020-01-18T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","The pump room natural vent head grating are rusty and need to remove them to carry out maintenance/replacement","Deck - Pipe / Fittings","General Appearance","Equipment Related,Inappropriate Procedure","","","","","Gratings removed and wire mesh renewed.Vent painted","2020-03-08T23:59:35","","Completed","2020-02-25T23:59:35","No","No","No","Internal"]
[null,null,null,10615,null,"53_28/02/2020 6:53:05 AM","2020-01-18T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","The main bunker tanks vent heads flanges are very rusty on port and stbd side of pump room. ","Deck - Pipe / Fittings","General Appearance","Equipment Related,Human Error,Inappropriate Procedure","","","","","Derusting and painting of bunker tank vent heads carried out.","2020-03-08T23:59:35","","Completed","2020-03-08T23:59:35","No","No","No","Internal"]
[null,null,null,10616,null,"53_28/02/2020 6:56:14 AM","2020-01-18T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","The aft side of the funnel is stained and need washing","Miscellaneous","General Appearance","Equipment Related","","","","","Aft Side of the funnel cleaned/ washed & stained removed.","2020-09-23T23:59:35","","Completed","2020-07-31T23:59:35","No","No","No","Internal","complete as planned and close out"]
[null,null,null,10617,null,"53_28/02/2020 7:01:51 AM","2020-01-18T23:59:35","Critical Equipment,Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","No spanners for Accommodation fire hose coupling opening/tightening","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","New spanners received & same put in use.","2020-07-23T23:59:35","DPUM200153","Completed","2020-07-08T23:59:35","No","No","No","Internal","spares processed for supply at Fuj"]
[null,null,null,10620,null,"53_28/02/2020 6:36:37 AM","2020-01-18T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Life boat propellers covered with metal casing though it is no longer required as per VIQ.","LSA / FFA","Safety / LSA / FFA","Human Error","","","","","Metal casings removed from propeller of port & stbd lifeboat","2020-01-20T23:59:35","","Completed","2020-01-19T23:59:35","No","No","No","Internal"]
[null,null,null,10621,null,"53_28/02/2020 6:40:02 AM","2020-01-18T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","The gears of windlass were found with lack of grease and window cover for greasing was hard to open.","Deck - Mooring Machinery","Mooring","Human Error,Inappropriate Procedure","","","","","Both windlass gears were greased and cover freed.","2020-01-20T23:59:35","","Completed","2020-01-19T23:59:35","No","No","No","Internal"]
[null,null,null,10213,null,"53_29/01/2020 10:26:33 AM","2020-01-20T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Ballast tank suction Pressure guages not show correct reading as compare to local guage. ","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.8","Medium","","","Calibration of gauges carried out","2020-02-08T23:59:35","","Completed","2020-01-27T23:59:35","No","No","No","Internal","vessel en route to Rastanura; kindly complete well prior arrival and clsoe out"]
[null,null,null,14120,null,"53_30/09/2020 4:58:20 AM","2020-01-23T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ER vent mushrooms to derust and paint","Miscellaneous","General Appearance","External Factors","10.29","Medium","","","Derusting and Painting of all ER mushroom vent completed.","2021-04-23T23:59:35","","Completed","2021-04-07T23:59:35","No","No","No","Internal","complete the rest and close out"]
[null,null,null,16526,null,"53_26/12/2020 3:38:43 PM","2020-01-24T23:59:35","Non Conformity","Ship Staff","Ship Staff Insp.","Connecting Pins for all mooring winch brake bands were painted and jammed","Deck - Mooring Machinery","Mooring","Behaviour Based","9.15","Medium","","","Pins for all mooring winches freed and lubricated.","2020-02-03T23:59:35","","Completed","2020-01-30T23:59:35","No","No","No","Internal"]
[null,null,null,10618,null,"53_17/02/2020 9:47:26 AM","2020-01-25T23:59:35","Observation","Ship Staff","Ship Staff Insp.","One no. Port gangway stonchion bracket cracked from weld seam","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","Equipment Related","5.47","Medium","","","COT 's purged,Concurrence taken from office,Stanchion weld seams repaired by hot work","2021-07-25T23:59:35","","Completed","2020-03-26T23:59:35","No","No","No","Internal","why is it deferred; kindly forward the pictures and the  alternate arrangement or plans for permanent repairs in separate mail"]
[null,null,null,10622,null,"53_17/02/2020 5:39:06 AM","2020-01-28T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Limit switch of starboard HHC hook found stuck","Deck - Machinery","Cargo / Ballast Systems","Equipment Related,Human Error","8.5","Very High","","","Limit switch overhauled,Lubrication of limit switch done","2020-01-29T23:59:35","","Completed","2020-01-28T23:59:35","No","No","No","Internal"]
[null,null,null,16527,null,"53_26/12/2020 3:57:08 PM","2020-01-28T23:59:35","Non Conformity","Ship Staff","Ship Staff Insp.","During pre arrival port checks,it was found that stbd HHC limit switches were stuck.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.5","Very High","","","Limit switches were overhauled and lubricated for port & stbd HHC.Both cranes tried out,found satisfactory.","2020-02-21T23:59:35","","Completed","2020-01-28T23:59:35","No","No","No","Internal"]
[null,null,null,10619,null,"53_28/02/2020 7:20:58 AM","2020-02-04T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Packing of all weathertight doors around accommodation found covered with paint and channels of doors rusted","Accommodation","General Appearance","Human Error,Knowledge Based","","","","","Packings of all weathertight doors removed and cleaned of paint marks,channels derusted and painted and packings fitted back.","2020-02-29T23:59:35","","Completed","2020-02-23T23:59:35","No","No","No","Internal","noted; crew to be educated not to paint the rubber packings"]
[null,null,null,11119,null,"53_29/03/2020 6:54:01 PM","2020-02-29T23:59:35","Observation","Ship Staff","Ship Staff Insp.","8 nos lashing wires for gangway broke during rough weather","Deck - Pipe / Fittings","Safety / LSA / FFA","External Factors","","","","","Accomodation ladder lashing wires received at fujairah & same replaced.New accomodation ladder lashing wires put in use.","2020-06-08T23:59:35","RO DPUM190172","Completed","2020-06-03T23:59:35","No","No","No","Internal","spares to be connected at Fujairah"]
[null,null,null,11124,null,"53_29/03/2020 6:44:09 PM","2020-02-29T23:59:35","Critical Equipment","Ship Staff","Ship Staff Insp.","Hoisting wire L1 of starboard Gangway found damaged during rough weather ","Deck - Machinery","Safety / LSA / FFA","External Factors","","","","","Hoisting wire L1 replaced with spare wire onboard.RO raised for spare wire DPUM200044","2020-03-08T23:59:35","","Completed","2020-03-02T23:59:35","No","No","No","Internal"]
[null,null,null,12735,null,"53_09/06/2020 12:29:37 PM","2020-03-02T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Cargo Audit","12.20.05.011.04 - Pre arrival and commencement of cargo operation\n\n checklist for loading at Charco Azul Sec B (24 Hrs Prior Operation)\n\n completed on 08 Apr at 1800 Hrs, however Operations commenced on\n\n 10 Apr 2020.Section B to be reviewed and re-signed in case \n\ncargo operations is delayed.\n\n","Miscellaneous","Cert. & Docu.","Behaviour Based,Human Error","8.1","Very High","","","CORRECTIVE ACTION: An observation has been made in the \n\nAudit / Assessment Report. A print of observation status has been\n\nfilled onboard for records in Audit / inspection report file.\n\n\n\n\n\nPREVENTIVE ACTION: All officers were briefed on the importance of \n\nupdating the checklist as & when task is completed / checked & \n\nrelevant entry to be made in CCR log book. This will avoid in \n\nfilling up checklist at last minute, which results in hastily \n\nmade wrong entries. Specific remarks to be added in checklist as \n\n& when appropriate.","2020-06-02T23:59:35","","Completed","2020-06-01T23:59:35","No","No","No","Internal"]
[null,null,null,12736,null,"53_14/06/2020 09:21:10","2020-03-02T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Bunkering Audit","Oil/Bunker transfering plan/Checklist/Procedures used onboard is an old version. ","Miscellaneous","Cert. & Docu.","Human Error,Inappropriate Procedure","","","","","All officers were briefed on the importance of using the latest amended checklist from PAL. Discussed the wrong practice carried out of saving the checklist in one place for easy access.\n\nAnd to download the checklist from Qdms pal system.","2020-06-08T23:59:35","","Completed","2020-06-01T23:59:35","No","No","No","Internal"]
[null,null,null,12737,null,"53_14/06/2020 09:30:43","2020-03-02T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Bunkering Audit","Bunker Transfer Plan / Checklist 12.04.08.011.01 Section 7 - Monitoring of H2S/Benzene Vapors : \n\nBenzene reading measured by detector tubes shall be mentioned < Min value that can be measured by the specific tube. For example by Gastec tubes Min measurable value is 0.05 ppm, hence in that case benzene shall be mention <0.05 ppm (if no discoloration observed)\n\nUnderstand vessel has kept the Gas tubes as evidence of monitoring.\n\n","Miscellaneous","Cert. & Docu.","Human Error,Inappropriate Procedure","","","","","An observation has been made in the Audit / Assessment Report. A print of observation status has been filled onboard for records in Audit / inspection report file.","2020-06-08T23:59:35","","Completed","2020-06-01T23:59:35","No","No","No","Internal"]
[null,null,null,12738,null,"53_14/06/2020 09:33:43","2020-03-02T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Bunkering Audit","12.04.08.014.00 Code \"A\" to be signed by both parties.","Miscellaneous","Cert. & Docu.","Human Error,Inappropriate Procedure","","","","","An observation has been made in the Audit / Assessment Report. A print of observation status has been filled onboard for records in Audit / inspection report file.","2020-06-08T23:59:35","","Completed","2020-06-01T23:59:35","No","No","No","Internal"]
[null,null,null,12739,null,"53_14/06/2020 09:37:05","2020-03-02T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Bunkering Audit","Repetitive checks were not carried out as per bunker safety checklist \n\nIt states repetitive checks to be carried every 0.5 hour, check list completed at 2215 hrs but repetitive check commenced at 0836 hrs. \n\n","Miscellaneous","Cert. & Docu.","Human Error,Inappropriate Procedure","","","","","An observation has been made in the Audit / Assessment Report. A print of observation status has been filled onboard for records in Audit / inspection report file.","2020-06-08T23:59:35","","Completed","2020-06-01T23:59:35","No","No","No","Internal"]
[null,null,null,11120,null,"53_03/04/2020 7:33:56 AM","2020-03-08T23:59:35","Observation","Ship Staff","Ship Staff Insp.","3 nos Angle bar supports for cow branch line for 1P COT fwd cow machine bent due to heavy weather","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","External Factors","","","","","COW branch line tested to 1.25 times working pressure,No damage to line integrity.Job to renew angle supports deffered to dry dock,refman job list exported to office on 6th apr","2021-09-24T23:59:35","","Completed","2020-03-30T23:59:35","No","No","No","Internal","planned for docking , awaiting ship's refman copy for repair specs"]
[null,null,null,11121,null,"53_03/04/2020 7:39:16 AM","2020-03-08T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Fwd bulkhead for Forepeak store entrance found with indentation of 2 cm due to heavy weather","Hull & Tanks","Structural Condn. / WT integrity ","External Factors","","","","","All weld seams cleaned and weld crack test done,None found,Starightening job deferred to Dry dock,refman export to office 6th apr 20","2021-07-25T23:59:35","","Completed","2020-03-30T23:59:35","No","No","No","Internal","forward the export copy of repair spec  for the refman"]
[null,null,null,11122,null,"53_03/04/2020 8:01:58 AM","2020-03-08T23:59:35","Defect","Ship Staff","Ship Staff Insp.","3 nos fire hose boxes damaged due to rough weather","LSA / FFA","Safety / LSA / FFA","External Factors","","","","","Spare fire hose boxes received at Fujairah. 3Nos. of Old broken fire hose boxes discarded & new fire hose boxes put in use.","2020-06-08T23:59:35","DPUM200049 ","Completed","2020-06-07T23:59:35","No","No","No","Internal","supply arranged at Fuj- end May"]
[null,null,null,11123,null,"53_03/04/2020 7:30:13 AM","2020-03-08T23:59:35","Observation","Ship Staff","Ship Staff Insp.","8 nos Stanchions for centre catwalk in forecastle area  bent during rough weather","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","External Factors","","","","","All stanchions removed from brackets and transferred to E/R workshop, straightened using hot work.","2020-04-10T23:59:35","","Completed","2020-04-06T23:59:35","No","No","No","Internal","to be completed and closed out at the earliest"]
[null,null,null,11125,null,"53_03/04/2020 7:45:25 AM","2020-03-08T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Guard cover for Port Anchor hawse pipe bent due to bad weather","Deck - Pipe / Fittings","General Appearance","External Factors","","","","","Guard cover removed from place and transferred to E/R workshop and straightened with hot work,and fitted back after repairs","2020-03-29T23:59:35","","Completed","2020-03-22T23:59:35","No","No","No","Internal"]
[null,null,null,11126,null,"53_03/04/2020 7:53:16 AM","2020-03-08T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Fwd Guard plate for FPK air vent bent due to rough weather","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","External Factors","","","","","Guard plate removed from place and taken to E/R workshop,Straightened using hot work and fitted back.","2020-03-29T23:59:35","","Completed","2020-03-22T23:59:35","No","No","No","Internal"]
[null,null,null,11127,null,"53_03/04/2020 8:10:35 AM","2020-03-08T23:59:35","Critical Equipment,Observation","Ship Staff","Ship Staff Insp.","Hydraulic lines for Port Anchor brake bent and lashing plates broken due to rough weather","Deck - Mooring Machinery,Deck - Pipe / Fittings","Mooring","External Factors","","","","","Lines opened and straightened in E/R workshop,fitted back and windlass tried out,New pipes ordered for renewal in future.RO-DPUM200049 Item 39","2020-03-13T23:59:35","","Completed","2020-03-11T23:59:35","No","No","No","Internal"]
[null,null,null,11128,null,"53_03/04/2020 7:42:16 AM","2020-03-08T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Safety guard rails for port side Anchor Hawse pipe uprooted from weld seams due to bad weather","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","External Factors","","","","","Hot work permit issued after concurrence from office,Safety rails repaired with hot work","2020-03-29T23:59:35","","Completed","2020-03-26T23:59:35","No","No","No","Internal"]
[null,null,null,11129,null,"53_03/04/2020 8:14:09 AM","2020-03-08T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Railings on fwd bulkhead of Fpk store entrance uprooted from weld seam due to rough weather","Deck - Pipe / Fittings","General Appearance","External Factors","","","","","Hot work permit issued after concurrence from office,Railings renewed ","2020-03-29T23:59:35","","Completed","2020-03-26T23:59:35","No","No","No","Internal"]
[null,null,null,11130,null,"53_03/04/2020 8:18:10 AM","2020-03-08T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Steel cable tie lashings for valve hydraulic lines on deck broken and hydraulic lines moved from location due to rough weather","Deck - Pipe / Fittings","Cargo / Ballast Systems","External Factors","","","","","Damaged steel ties renewed and all hydraulic lines at place.All hydraulic valves tried out,All in good working order","2020-03-12T23:59:35","","Completed","2020-03-10T23:59:35","No","No","No","Internal"]
[null,null,null,11131,null,"53_03/04/2020 7:49:50 AM","2020-03-08T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Fwd plate and top protection cover for fwd ETA chain bent due to bad weather ","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","External Factors","","","","","Top cover and Fwd plate for ETA opened from bolts and taken to E/R workshop and straightened using hot work.Covers fitted back.","2020-03-29T23:59:35","","Completed","2020-03-26T23:59:35","No","No","No","Internal"]
[null,null,null,11135,null,"53_03/04/2020 8:24:10 AM","2020-03-08T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Weld seam of 1 no. Stanchion of starboard gangway broken","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","External Factors","","","","","Hot work permit issed after concurrence with office,Weld seam repaired","2020-03-29T23:59:35","","Completed","2020-03-26T23:59:35","No","No","No","Internal"]
[null,null,null,11132,null,"53_03/04/2020 8:57:17 AM","2020-03-09T23:59:35","Critical Equipment,Observation","Ship Staff","Ship Staff Insp.","3 nos expansion joints found leaking on fire line","LSA / FFA","Safety / LSA / FFA","Equipment Related,External Factors","","","","","Bolts tightened,Leaks not arrested,Expansion joints opened,6 nos rubber packings renewed.Line tested ,No leaks,RO raised for spare rubber packings.","2020-03-13T23:59:35","","Completed","2020-03-12T23:59:35","No","No","No","Internal"]
[null,null,null,11133,null,"53_03/04/2020 8:40:44 AM","2020-03-10T23:59:35","Critical Equipment,Observation","Ship Staff","Ship Staff Insp.","6 Nos of Expansion joints on cargo lines found leaking after pressure testing,Leaks not arrested after tightening of bolts","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","All 6 expansion joints opened,surfaces cleaned,6 rubber packings renewed.Cargo lines pressure tested to 12.5 bars,No leaks.RO raised for new rubber packings DPUM200059","2020-03-12T23:59:35","","Completed","2020-03-12T23:59:35","No","No","No","Internal"]
[null,null,null,11134,null,"53_03/04/2020 8:32:39 AM","2020-03-11T23:59:35","Critical Equipment","Ship Staff","Ship Staff Insp.","Comm.error for 1P,5P & 5S Pressure sensors for COT","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","Pressure sensors checked by ETO,zero calibration done,all connections checked,system restarted,error exists for 1P & 5P.1P & 5P pressure sensors renewed.","2020-03-12T23:59:35","","Completed","2020-03-12T23:59:35","No","No","No","Internal"]
[null,null,null,16528,null,"53_26/12/2020 8:03:40 PM","2020-03-24T23:59:35","Non Conformity","Ship Staff","Ship Staff Insp.","Rest hour violation for less than 10 hrs in any 24 hrs period ","Miscellaneous","Crew Management","External Factors","3.2","Very High","","","Compensatory rest of 12 hrs was given immediately after rest hour violation. ","2020-04-23T23:59:35","","Completed","2020-03-29T23:59:35","No","No","No","Internal"]
[null,null,null,11407,null,"53_15/04/2020 10:43:40 PM","2020-03-27T23:59:35","Critical Equipment","Ship Staff","Ship Staff Insp.","Operating lever for engaging gear of stbd windlass broken.","Deck - Mooring Machinery","Mooring","Equipment Related","","","","","Stainless steel bolt was machined and fitted in place of operating lever.Windlass was tried out. All satisfactory","2020-09-25T23:59:35","","Completed","2020-09-21T23:59:35","No","No","No","Internal","check the condition / play in other winches also and revert. spares processed for supply// spares arranged for supply"]
[null,null,null,11406,null,"53_15/04/2020 10:35:06 PM","2020-04-01T23:59:35","Critical Equipment","Ship Staff","Ship Staff Insp.","During pre arrival port checks,it was noticed that the horn for hi alarm for CCR anemometer was not working on monkey island.Flashing light was in working condition.Audio & Visual alarm in CCR in working condition.","Elect. Mach. & Equip.","Safety / LSA / FFA","Equipment Related,External Factors","","","","","renewed with new spares recieved","2020-05-24T23:59:35","","Completed","2020-06-19T23:59:35","No","No","No","Internal","PO reference should be in correct box.  Kindly follow up key issues in separate mail so there is no lag in information. spares will be process on priority. send reminder to purchase for the spares required at next port of call."]
[null,null,null,16529,null,"53_26/12/2020 7:56:05 PM","2020-04-05T23:59:35","Non Conformity","Ship Staff","Ship Staff Insp.","Minimum total rest comprises more than 2 periods","Miscellaneous","Crew Management","External Factors","3.2","Very High","","","Compensatory rest of 12 hrs was given immediately after rest hour violation. ","2020-05-23T23:59:35","","Completed","2020-05-02T23:59:35","No","No","No","Internal"]
[null,null,null,11692,null,"53_06/05/2020 13:20:30","2020-04-09T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Elevator inoperational due to safty gear.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","External Factors","","","","","Elevator made operational","2020-05-24T23:59:35","","Completed","2020-04-26T23:59:35","No","No","No","Internal","serv to arrange at the next available port of call.\ncouldn't fix with remote assistance.\nvessel to raise serv RO and mention under PO reference"]
[null,null,null,11693,null,"53_06/05/2020 8:27:30 PM","2020-04-11T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Two 12 mm BWTS sample  lines for TRO sensor in pumproom found holed from various places.Length of each line approx. 8mtrs. ","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","Both lines removed & taken to E/R workshop,Lines found beyond repair.New lines fabricated & fitted back in pumproom.","2020-04-23T23:59:35","","Completed","2020-04-15T23:59:35","No","No","No","Internal"]
[null,null,null,11694,null,"53_06/05/2020 8:32:55 PM","2020-04-12T23:59:35","Critical Equipment","Ship Staff","Ship Staff Insp.","Stripper line valve for 3C COT not operational from CCR panel","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","Coils for solenoid valve found faulty,same renewed.Valve tried out,working satisfactorily.","2020-04-13T23:59:35","","Completed","2020-04-12T23:59:35","No","No","No","Internal"]
[null,null,null,16530,null,"53_26/12/2020 7:37:42 PM","2020-04-17T23:59:35","Non Conformity","Ship Staff","Ship Staff Insp.","Smoke detector isolated from local panel for Workshop welding area without master permission and without informing bridge OOW. ","LSA / FFA","Safety / LSA / FFA","Inappropriate Procedure","5.35","Medium","","","Immediately called Engine control room and Ask to Engineer to stop the welding work in workshop and Smoke detecting was made normal. and job was restarted after proper risk assessment. ","2020-05-23T23:59:35","","Completed","2020-05-01T23:59:35","No","No","No","Internal"]
[null,null,null,16531,null,"53_26/12/2020 6:41:45 PM","2020-05-02T23:59:35","Non Conformity","Ship Staff","Ship Staff Insp.","During routine inspection of laundries,metallic items and tools were found inside the washing machine alongwith boiler suits.","Accommodation","General Appearance","Behaviour Based","11.14","Medium","","","Washing machine was stopped and metallic parts and tools removed.","2020-05-23T23:59:35","","Completed","2020-05-23T23:59:35","No","No","No","Internal"]
[null,null,null,11931,null,"53_18/05/2020 6:35:29 PM","2020-05-02T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Brass regulator for charging lifeboat Air Bottle Cylinder with pressure gauge found missing.","LSA / FFA","Safety / LSA / FFA","Human Error","5.28","Very High","","","DPUM200193 received on 22 Sep 2020 @ Singapore, Brass regulator for charging lifeboat bottle cylinder kept in safety locker & stencilled.","2020-10-01T23:59:35","DPUM200193","Completed","2020-09-15T23:59:35","No","No","No","Internal","arranged and expected connection at Fuj - end May"]
[null,null,null,11974,null,"53_20/05/2020 4:15:10 PM","2020-05-13T23:59:35","Defect","Ship Staff","Ship Staff Insp.","CO 2 bottles securing clamp cracked","Critical Equip.","Structural Condn. / WT integrity ","External Factors","","","","","spare recieved same renewed","2020-06-08T23:59:35","DPUM205023","Completed","2020-06-05T23:59:35","No","No","No","Internal","spares arranged, awaiting connection"]
[null,null,null,11975,null,"53_20/05/2020 4:22:32 PM","2020-05-13T23:59:35","Critical Equipment","Ship Staff","Ship Staff Insp.","Emergency generator batery charger source fail alarm","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","Reciewed Two Spare SCR's , one PCB & 2 Relays 24 VOLT dc same replaced working satisfactory.","2020-07-23T23:59:35","DPUM200120","Completed","2020-06-18T23:59:35","No","No","No","Internal","spares confirmed for supply, will be connected  on priority soon.. battery monitored on daily basis"]
[null,null,null,11976,null,"53_29/05/2020 17:19:11","2020-05-19T23:59:35","Defect","Ship Staff","Ship Staff Insp.","E.R Crane 20 core cable from starter box to traversing block showing open circuit in 3 core.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.28","Low","","","Recieved spare 20 core cable same replaced with proper securing arrangemet.","2020-06-03T23:59:35","DPUM200135","Completed","2020-06-11T23:59:35","No","No","No","Internal","spares to be arranged on priority"]
[null,null,null,11977,null,"53_29/05/2020 17:30:21","2020-05-21T23:59:35","Defect","Ship Staff","Ship Staff Insp.","No.2 electric ballast pump filter inlet valve (BA038) is not showing valve position in BWTS display.","Elect. Mach. & Equip.","Cargo / Ballast Systems","Equipment Related","6.21","High","","","Following maker's instruction, valve simulated for open and shut. put back in auto. presently working.","2020-08-24T23:59:35","","Completed","2020-10-02T23:59:35","No","No","No","Internal","troubleshooting ongoing with makers; followup serv will be  engaged  at next convenient port if unable to resolve remotely // PCB arranged for supply// awaiting convenient port for ser attendance- Covid travel restrictions in China"]
[null,null,null,11979,null,"53_31/05/2020 12:56:30 PM","2020-05-21T23:59:35","Critical Equipment,Defect","Ship Staff","Ship Staff Insp.","During routine inspection it was found that stbd Accomodation ladder shifting wire - L2 has a twist & damage.","Deck - Machinery","ISM Related","Equipment Related,External Factors","5.47","Medium","","","New shifting wire received at fujairah & same put in use , Old damaged shifting wire\"L2\" discarded.","2020-08-20T23:59:35","DPUM 200140","Completed","2020-06-02T23:59:35","No","No","No","Internal","RO received ;  spares to be arranged on priority"]
[null,null,null,12717,null,"53_13/06/2020 02:05:06","2020-05-25T23:59:35","Defect","Ship Staff","Ship Staff Insp.","ME all unit one blank flange from the liner jacket has salt dposits depicting leakages, though presently no flowing /dripping water observed.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","All unit liner jacket inlet and outlet valve to isolate drain and gasket renewed","2020-08-05T23:59:35","","Completed","2020-08-13T23:59:35","No","No","No","Internal","to be taken up at the next convenient anchorage on priority"]
[null,null,null,12718,null,"53_13/06/2020 02:10:21","2020-05-25T23:59:35","Defect","Ship Staff","Ship Staff Insp.","ME unit #1 accumulator block leaking badly.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","O-rings renewed and tightened to torque","2020-08-08T23:59:35","","Completed","2020-08-21T23:59:35","No","No","No","Internal","to be overhauled on priority at the next available anchorage"]
[null,null,null,12719,null,"53_13/06/2020 02:13:09","2020-05-25T23:59:35","Defect","Ship Staff","Ship Staff Insp.","ME unit# 1 lo leakges present from the bottom of both FO booster and actuator unit.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","O-rings renewed and tightened to 2200bars","2020-08-08T23:59:35","","Completed","2020-08-24T23:59:35","No","No","No","Internal","to be overhauled on priority at the next available anchorage"]
[null,null,null,12720,null,"53_13/06/2020 02:18:47","2020-05-25T23:59:35","Defect","Ship Staff","Ship Staff Insp.","ME unit# 2 FO booster and actuator bottom leaking of LO.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","O-rings renewed and tightened to 2200bars","2020-08-08T23:59:35","","Completed","2020-08-24T23:59:35","No","No","No","Internal","to be overhauled on priority at the next available anchorage"]
[null,null,null,12721,null,"53_13/06/2020 02:25:11","2020-05-25T23:59:35","Defect","Ship Staff","Ship Staff Insp.","ME unit #1 LDCL liner i/l drain pipe has deposits depicting leakages which might have been arrested because of deposits itself.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","isolate the unit #1 jacket water inlet/outlet valve.Drain the system.retighten the pipe union  line.","2020-12-08T23:59:35","","Completed","2020-08-13T23:59:35","No","No","No","Internal"]
[null,null,null,12722,null,"53_13/06/2020 02:29:58","2020-05-25T23:59:35","Defect","Ship Staff","Ship Staff Insp.","ME unit #5 allen bolt for acuator keeps losening due to vibration, and permanently an allen key is tied to it to keep it in place.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Isolate the system.Allen bolt and hole threads cleaned. tightenend with thread lock","2020-06-28T23:59:35","","Completed","2020-08-13T23:59:35","No","No","No","Internal","to be overhauled on priority at the next available anchorage"]
[null,null,null,12723,null,"53_13/06/2020 02:51:55","2020-05-25T23:59:35","Observation","Ship Staff","Ship Staff Insp.","ME # 1 FO supply pump motor needs overhauling.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","MOTOR OVERHAULED WITH NEW BEARINGS","2020-07-08T23:59:35","","Completed","2020-06-24T23:59:35","No","No","No","Internal","complete as per target date and close out"]
[null,null,null,12724,null,"53_13/06/2020 02:56:27","2020-05-25T23:59:35","Observation","Ship Staff","Ship Staff Insp.","LT cooler #1  sacrificial flange is leaky.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","sacrificial flange renewed","2020-12-08T23:59:35","","Completed","2020-06-30T23:59:35","No","No","No","Internal"]
[null,null,null,12725,null,"53_13/06/2020 03:01:14","2020-05-25T23:59:35","Defect","Ship Staff","Ship Staff Insp.","ME maoti filter distributer unit is damaged and found welded, Will have to fit in place and check for the operability.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related,Inappropriate Procedure","10.32","Very High","","","Tried using the spare maoti filter complete assembly after few minutes fouund the assembly was stuck not rotating","2020-12-08T23:59:35","","Completed","2020-08-17T23:59:35","No","No","No","Internal","the spares are processed as per ship's feedback.\nexcept the element set rest others processed for supply. include the RO in the DDRL"]
[null,null,null,12726,null,"53_13/06/2020 03:08:57","2020-05-25T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Stbd Fwd bunker manifold valve stuck / jammed in shut position.","Deck - Pipe / Fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Overhauling of valve carried out eased and greased  now operating properly.                       Job  no:V-DPUM027859/20","2020-08-23T23:59:35","","Completed","2020-07-28T23:59:35","No","No","No","Internal","complete and close out as per target date.\nshould have being completed by now."]
[null,null,null,12727,null,"53_13/06/2020 03:14:35","2020-05-25T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Composite boiler FW pump seal is leaky.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","New mechanical seal recived and assembled on pump. Pump operational now.","2020-07-08T23:59:35","DPUM200109","Completed","2020-11-09T23:59:35","No","No","No","Internal","Seal will be processed in the mean time inspect the seal; it is likely that the O'Ring is hardened and require replacement."]
[null,null,null,12728,null,"53_14/06/2020 08:37:05","2020-05-25T23:59:35","Defect","Ship Staff","Ship Staff Insp.","FWG ejector pump mechanical seal leaking.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Spare recieved and same replaced no leak.","2020-06-08T23:59:35","","Completed","2020-06-08T23:59:35","No","No","No","Internal","kindly attend while sailing if the valves are holding"]
[null,null,null,12729,null,"53_14/06/2020 08:41:10","2020-05-25T23:59:35","Defect","Ship Staff","Ship Staff Insp.","M.C.S.W Pump no # 1 mechanical seal leaking.","E/R - Pumps","Emgcy. Systems","Equipment Related","","","","","RENEWED WITH NEW SEALS","2020-07-08T23:59:35","DPUM200128","Completed","2020-07-06T23:59:35","No","No","No","Internal","complete the job as planned and close out. Raise RO for the spares consumed."]
[null,null,null,12730,null,"53_14/06/2020 12:42:59","2020-05-25T23:59:35","Observation","Ship Staff","Ship Staff Insp.","STBD provision crane limit switches not operating.","Deck - Machinery","Cargo / Ballast Systems","Equipment Related","","","","","Received spare in singapore.Replaced the limit switch with new spare.Tried out working satisfactory.Job no:V-DPUM028637/20","2020-07-08T23:59:35","DPUM200188","Completed","2020-09-19T23:59:35","No","No","No","Internal","spares processed; kindly complete the job once they are connected to ship.."]
[null,null,null,12731,null,"53_14/06/2020 12:46:28","2020-05-25T23:59:35","Defect","Ship Staff","Ship Staff Insp.","gas detction system triping on System trips on pump internal leakage.","Elect. Mach. & Equip.","Cargo / Ballast Systems","Equipment Related","5.21","Medium","","","Flame arrestor cleaned .pipe cleared. No more system trips working satisfactroy.","2020-07-08T23:59:35","","Completed","2020-06-08T23:59:35","No","No","No","Internal","awaiting further details; revert with separate mail if makers assistance is required"]
[null,null,null,12740,null,"53_13/06/2020 02:44:19","2020-05-25T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Auxiliary Engine # 3 priming LO pump motor needs overhauling","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Motor overhauled bearing renewed.job updated in PMS","2020-06-08T23:59:35","","Completed","2020-06-04T23:59:35","No","No","No","Internal"]
[null,null,null,12741,null,"53_13/06/2020 03:17:55","2020-05-25T23:59:35","Observation","Ship Staff","Ship Staff Insp.","OIly bilge pump unable to transfer bilge water to sludge collecting tank and oily bilge tank. Needs investigation. (probably common valve needs to be checked).","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","valve opened found stuck same eased up and tried. now able to transfer to sludge collecting tank.","2020-07-08T23:59:35","","Completed","2020-06-03T23:59:35","No","No","No","Internal"]
[null,null,null,12742,null,"53_14/06/2020 08:32:46","2020-05-25T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Scrubber pump mechanical seal leaking.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Removed the motor and coupling. Removed the mechanical seal stationary part rotating part spring found stuck same eased up and tried out found no leak.","2020-07-08T23:59:35","","Completed","2020-06-06T23:59:35","No","No","No","Internal"]
[null,null,null,12743,null,"53_14/06/2020 08:48:29","2020-05-25T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Provision refer compressor #1 was not in use oil charging valve was jammed. ","Elect. Mach. & Equip.,Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Isolated the system removed the oil charging valve same eased up checked the operation and oil topped up. working satisfactory.","2020-07-08T23:59:35","","Completed","2020-06-06T23:59:35","No","No","No","Internal"]
[null,null,null,12744,null,"53_14/06/2020 09:49:28","2020-05-25T23:59:35","Defect","Ship Staff","Ship Staff Insp.","A.E#2 L.O priming motor abnormal sound and vibration.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Motor overhauled and bearing renewed.","2020-06-08T23:59:35","","Completed","2020-06-01T23:59:35","No","No","No","Internal"]
[null,null,null,12745,null,"53_14/06/2020 12:39:58","2020-05-25T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Incinerator safties were bypassed.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related,Inappropriate Procedure","","","","","All safeties put back to normal tried out all working satisfactory.","2020-06-07T23:59:35","","Completed","2020-05-28T23:59:35","No","No","No","Internal"]
[null,null,null,11978,null,"53_31/05/2020 1:14:57 PM","2020-05-26T23:59:35","Defect","Ship Staff","Ship Staff Insp.","It was observed that the port Anchor flukes are not resting on hawse pipe lips when anchor is stowed & secured in position.","Deck - Mooring Machinery","Mooring","Equipment Related","9.2","Very High","","","Vessel attempted to remove the twist from anchor cable on 26 Jun 2020 at Qingdao OuterAnchorage but to No avail Flukes are still not resting on the Bulb for stowing. As suggested by Operations vessel is taking additional lashing on port anchor during laden passage.Job deffered for DD, same to be added in Refman","2021-08-25T23:59:35","","Completed","2021-02-04T23:59:35","No","No","Yes","Internal",""]
[null,null,null,12732,null,"53_09/06/2020 12:16:49 PM","2020-05-27T23:59:35","Defect","Ship Staff","Ship Staff Insp.","No.2 COP Suction valve & pumproom bulkhead master valve leaking.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.21","High","","","Observed during loaded passage & found no passing on the suction & bulkhead master valves. It could have been because at earlier voyage bottom lines might not have been well stripped.","2020-09-23T23:59:35","","Completed","2020-07-29T23:59:35","No","No","No","Internal","awaiting further update. check the seat ring stock."]
[null,null,null,16532,null,"53_26/12/2020 6:57:16 PM","2020-05-28T23:59:35","Non Conformity","Ship Staff","Ship Staff Insp.","ORB Part I & II each entry is not counter signed in accordance with Fleet Memo HSQE/002/2020 16 Jan 2020.","Documentation","Cert. & Docu.","Human Error","2.1","Very High","","","An NCN has been made in the PAL LPSQ module, & all officers Re-briefed on the Fleet Memo HSQE/002/2020 16 Jan 2020.","2020-06-23T23:59:35","","Completed","2020-06-07T23:59:35","No","No","No","Internal"]
[null,null,null,12746,null,"53_15/06/2020 9:39:15 AM","2020-05-28T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Cargo Audit","ORB Part I & II each entry is not counter signed in accordance with Fleet Memo HSQE/002/2020 16 Jan 2020.\n\n","Documentation","Cert. & Docu.","Behaviour Based,Human Error","2.1","Very High","","","An NCN has been made in the PAL LPSQ module, & all officers Re-briefed on the Fleet Memo HSQE/002/2020 16 Jan 2020.","2020-06-23T23:59:35","","Completed","2020-06-07T23:59:35","No","No","No","Internal"]
[null,null,null,12733,null,"53_14/06/2020 08:52:52","2020-05-30T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Main central cooling F.W sysytem  valve no 44V non return valve not holding","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","To renew the valve.LT WATER NEEDS TO BE DRAINED TILL VALVE LEVEL. IT WILL BE A BLACK OUT JOB.TO BE DONE AS PER THE AVAILABILITY OF TIME OR DURING DRY DOCKING. INCLUDED IN REFMAN FOR DD.","2020-12-08T23:59:35","DPUM200234","Completed","2020-12-08T23:59:35","Yes","No","No","Internal","kindly raise defect for docking and close out in DDRL"]
[null,null,null,12734,null,"53_14/06/2020 08:56:51","2020-05-30T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Main central cooling F.W system  valve no 14 V leaking.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","To overhauled or renew the valve with new spare.LT WATER NEEDS TO BE DRAINED TILL VALVE LEVEL. IT WILL BE A BLACK OUT JOB.TO BE DONE AS PER THE AVAILABILITY OF TIME OR DURING DRY DOCKING. (INCLUDED IN REFMAN)","2020-12-08T23:59:35","","Completed","2020-12-08T23:59:35","Yes","No","No","Internal","Raise RO as well if it is butterfly valve ; in case the replacement is required"]
[null,null,null,12747,null,"53_09/06/2020 12:23:36 PM","2020-05-30T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Fire & Foam line Isolation valves are very hard in opening.Total : 7 Valves","Deck - Pipe / Fittings,LSA / FFA","Safety / LSA / FFA","Behaviour Based,Equipment Related,External Factors","5.38","High","","","Easing up & lubrication of  Fire & foam line isolation valves carried out & all 7 Fire/ Foam isolation valves are eased up.","2020-06-23T23:59:35","","Completed","2020-06-07T23:59:35","No","No","No","Internal"]
[null,null,null,12850,null,"53_30/06/2020 10:17:30 AM","2020-06-08T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Elevator door inverter malfunctioning.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Elevator door inverter replace with new spare and programmed.All the parameters from old inverter copied to new spare.                                                 Job no:V-DPUM028642/20","2020-07-22T23:59:35","DPUM200155","Completed","2020-09-19T23:59:35","No","No","No","Internal","spares processed/ please follow-up and confirm status"]
[null,null,null,12855,null,"53_22/06/2020 8:29:50 AM","2020-06-08T23:59:35","Defect,Observation","Ship Staff","Ship Staff Insp.","AIS observed giving TX power down alarm. ","Navigation - DGPS / EPFS / AIS","Navigation","Equipment Related,External Factors","","","","","New transponder ordered and installed on 05 June 2020 by Maritronics tech. System working satisfactory now. ","2020-06-23T23:59:35","","Completed","2020-06-08T23:59:35","No","No","No","Internal"]
[null,null,null,12856,null,"53_22/06/2020 8:38:45 AM","2020-06-08T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Old versions of Master’s Night order book and Compass Error Book were still in use. ","Documentation","Cert. & Docu.","Human Error,Inappropriate Procedure","","","","","Closed out the old books and new logbooks started.     ","2020-06-23T23:59:35","","Completed","2020-06-08T23:59:35","No","No","No","Internal"]
[null,null,null,12859,null,"53_22/06/2020 8:19:45 AM","2020-06-08T23:59:35","Critical Equipment,Observation","Ship Staff","Ship Staff Insp.","In use Mag. Compass observed to have large bubble as liquid has been leaking from compass. ","Critical Equip.,Navigation - Others","Navigation","Human Error,Inappropriate Procedure,Knowledge Based","4.9","Medium","","","Replaced with spare unit during Class annuals in Fujairah on 05 June 2020. Spare liquid and plugs placed on order. Once received shall rectify the spare magnetic compass.     ","2020-06-23T23:59:35","DPUM205040","Completed","2020-06-08T23:59:35","No","No","No","Internal"]
[null,null,null,12851,null,"53_30/06/2020 10:08:43 AM","2020-06-09T23:59:35","Defect","Ship Staff","Ship Staff Insp.","L.O cooler controller defective .","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","New spare LO controller installed, working satisfactory.","2020-08-23T23:59:35","DPUM200161","Completed","2020-11-02T23:59:35","No","No","No","Internal","spares to be arranged and connected"]
[null,null,null,12857,null,"53_30/06/2020 10:03:10 AM","2020-06-09T23:59:35","Observation","Ship Staff","Ship Staff Insp.","L.T cooler,FWG controller and M.E JCFW controller have some error in control position in the controller and remote position.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Calibration of controllers carried out .working satisfactory.","2020-06-23T23:59:35","","Completed","2020-06-20T23:59:35","No","No","No","Internal"]
[null,null,null,14463,null,"53_28/10/2020 3:24:24 PM","2020-06-10T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","Forward Hydraulics -- Section of cooling water inlet line leaking with pin hole","Deck - Mooring Machinery,Deck - Pipe / Fittings","General Appearance","Equipment Related","11.4","Very High","","","Section of pipe removed, Repaired & put back in place; Job Order No.--- V-DPUM029244/20","2020-06-13T23:59:35","","Completed","2020-06-10T23:59:35","No","No","No","Internal"]
[null,null,null,12853,null,"53_23/06/2020 11:43:28 PM","2020-06-16T23:59:35","Observation","Ship Staff","Ship Staff Insp.","With reference to onboard CCTV cameras installation, vessel is suppose to be fitted with CCTV IR type cameras particularly on following locations. \n\n1) 2 nos in Bridge (Facing BCC and Radio/Chart tables).\n\n2) 1 no in Cargo control room facing Cargo Console.\n\n3) 2 nos. in ECR (Facing switch board and ECR Console. \n\n4) 1 no. mid section of bridge facing deck area to cover entire deck (if camera is not fitted on bridge wings).\n\n5) 1 no inside scrubber housing (if vessel fitted with scrubber). Out of the above locations vessel is fitted with cameras only inside bridge as per \"1) 2 nos in Bridge (Facing BCC and Radio/Chart tables)\".","Miscellaneous","General Appearance","Equipment Related","","","","","cctv already installed, commisioning in progress","2021-01-23T23:59:35","DPUM205057: CCTV SYSTEM HARDWARE PACKAGE (generated by Office).","Completed","2021-01-08T23:59:35","No","No","No","Internal","Request commissioning guidelines and complete the job"]
[null,null,null,12854,null,"53_30/06/2020 10:17:17 AM","2020-06-16T23:59:35","Defect","Ship Staff","Ship Staff Insp.","During Pre- Arrival Cargo pressure testing observed 3 COW machine valves are passing, Namely 1C - No. 4; 2P - No.2 & Slp S - No.1.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.21","High","","","Slp S, 2P & 1C COW  machine valve seat ring renewed.","2020-08-24T23:59:35","DPUM200183","Completed","2020-07-30T23:59:35","No","No","No","Internal","to be completed and updated in weekly reports under additional sheet once the spares are received"]
[null,null,null,12858,null,"53_30/06/2020 9:47:08 AM","2020-06-18T23:59:35","Observation","Ship Staff","Ship Staff Insp.","When using emergency steering it was observed from NO 2 steering motor when order was given,afer few seconds the rudder starts moving not able to hold position.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.39","High","","","Zero position adjustment done. tried out emergency steering now working satisfactory.","2020-06-23T23:59:35","","Completed","2020-06-21T23:59:35","No","No","No","Internal"]
[null,null,null,14461,null,"53_30/10/2020 8:08:00 AM","2020-06-21T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Steering gear system alarms indication not coming on BCC, though they are being recorded on AMS panel in ECR","Elect. Mach. & Equip.,Navigation - Others","Eng. / Strg. Comp.","Equipment Related","10.39","High","","","Service engineer visited at Yeosu anchorage and circuit modification was carried out, now operational","2021-01-08T23:59:35","DPUM200284","Completed","2021-01-07T23:59:35","No","No","No","Internal","new spare supplied and  still the issue is open. maker serv to  be engaged at forthcoming discharge port Korea"]
[null,null,null,13168,null,"53_14/07/2020 18:31:37","2020-06-29T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","MOTOR BURNED DUE TO BEARING HOUSING NON DRIVING END GOT DAMAGED AND STATOR AND ROTOR CAME IN CONTACT","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","NEW MOTOR RECIEVED SAME INSTALLED NOW WORKING IN GOOD CONDITION","2020-07-08T23:59:35","DPUM200185","Completed","2020-07-05T23:59:35","No","No","No","Internal"]
[null,null,null,16533,null,"53_26/12/2020 8:52:45 PM","2020-07-03T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ISM: Each Winch greasing points were highlighted by yellow colored paint but same were not numbered. ","Deck - Mooring Machinery","Mooring","Human Error","9.2","Very High","","","All mooring winch greasing points cleaned, Highlighted with yellow paint, same numbered & stencil in place.","2020-10-02T23:59:35","","Completed","2020-08-09T23:59:35","No","No","No","Internal"]
[null,null,null,16534,null,"53_26/12/2020 9:04:00 PM","2020-07-03T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","MLC: Following two issues noted in Ship's Laundry:\n\n1. One drier air filter found covered with lint.\n\n2. Possible leakage noted at blower as water droplets were noted.","Accommodation","General Appearance","Behaviour Based,External Factors","11.14","Medium","","","1.Crew Re-Briefed about the importance of cleaning the filter before using the Dryers. Same been frequently checked for compliance & found in order.     \n\n2.Ships laundry panel opened up & pinhole leaking FW pipe repaired & leakage of water stopped.        ","2020-10-02T23:59:35","","Completed","2020-07-09T23:59:35","No","No","No","Internal"]
[null,null,null,16536,null,"53_26/12/2020 8:58:20 PM","2020-07-03T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ISPS: Port anchor in use. Although hawse pipe cover was in place, same was not secured.","Deck - Mooring Machinery","ISPS Related","Human Error","7.12","High","","","New securing arrangemet made for securing of the Hawse pipe when anchor is in use, Same kept in Focsle store & stencilled.","2020-10-02T23:59:35","","Completed","2020-07-21T23:59:35","No","No","No","Internal"]
[null,null,null,13255,null,"53_19/07/2020 15:07:18","2020-07-03T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Rough weather damage to cable tray on main deck, job not well executed. Kindly redo the lashings and use some Teflon to protect the sheathing.","Deck - Machinery","General Appearance","Equipment Related,External Factors","10.29","Medium","","","Lashings renewed on cable tray with Teflon sheet underneath.","2020-10-02T23:59:35","","Completed","2020-09-18T23:59:35","No","No","No","Internal","job to be completed as planned and close out"]
[null,null,null,13256,null,"53_19/07/2020 15:05:34","2020-07-03T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Both windlass cosmetics to improve","Deck - Machinery","General Appearance","Equipment Related","10.29","Medium","","","Derusting & painting of Port & Stbd windlass completed.","2020-09-23T23:59:35","","Completed","2020-09-21T23:59:35","No","No","No","Internal","job to be completed as planned and close out"]
[null,null,null,13257,null,"53_19/07/2020 12:46:50","2020-07-03T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Pump room blower suction filter mesh to repair","Deck - Machinery","Cargo / Ballast Systems","Equipment Related","11.4","Very High","","","Two different types of mesh currently fitted, R.O raised for suitable mesh and shall replace once received.         RO NO.DPUM200207, Item added in SIR – work list 22 Sep 2020 as vessel still awaiting spares.","2020-09-23T23:59:35","DPUM200207","Completed","2020-09-15T23:59:35","No","No","No","Internal","job to be completed as planned and close out; spare mesh will be supplied as per the RO"]
[null,null,null,13258,null,"53_19/07/2020 12:49:01","2020-07-03T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Main deck crossover platforms to remove and carry out cosmetic maintenance","Deck - Machinery","Cargo / Ballast Systems","Equipment Related","11.4","Very High","","","Derusting & painting of crossover platforms completed.","2020-09-23T23:59:35","","Completed","2020-09-20T23:59:35","No","No","No","Internal","job to be completed as planned and close out"]
[null,null,null,13259,null,"53_19/07/2020 12:54:23","2020-07-03T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Deck hydraulic line isolation handles corroded","Deck - Machinery","General Appearance","Equipment Related,External Factors","11.4","Very High","","","Deck Hydraulic line isolation valve handles derusted & Painted.","2020-08-23T23:59:35","","Completed","2020-07-29T23:59:35","No","No","No","Internal","job to be completed as planned and close out"]
[null,null,null,13260,null,"53_19/07/2020 13:04:50","2020-07-03T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Accommodation stores to be cleaned and scope of better arrangement","Accommodation","General Appearance","Behaviour Based,External Factors","10.29","Medium","","","All accommodation stores cleaned & arranged","2020-09-23T23:59:35","","Completed","2020-08-06T23:59:35","No","No","No","Internal"]
[null,null,null,13261,null,"53_19/07/2020 13:08:19","2020-07-03T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Stbd gangway stowing wires to renew and greasing points to be marked","Deck - Machinery","Cargo / Ballast Systems","Equipment Related","11.4","Very High","","","Port & Stbd Gangway stowing wire Degreased, cleaned, inspected, lubricated & put back in use; gangway wire is in good condition. Greasing points for gangway highlighted with yellow paint & numbering carried out for greasing points.","2020-08-23T23:59:35","","Completed","2020-08-13T23:59:35","No","No","No","Internal","job to be completed as planned and close out"]
[null,null,null,13262,null,"53_19/07/2020 13:21:06","2020-07-03T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Port windlass brake control hydraulic lines not as per original layout and not well secured.","Deck - Machinery,Deck - Pipe / Fittings","Mooring","Equipment Related,External Factors","10.29","Medium","","","Renewed the pipe fittings in various places and pipe bended to the original lay out.Tried the operation of windlass no leakages and operating satisfactory.Job no:V-DPUM028638/20","2020-08-23T23:59:35","DPUM200202","Completed","2020-09-21T23:59:35","No","No","No","Internal"]
[null,null,null,13263,null,"53_19/07/2020 13:24:54","2020-07-03T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Forecastle store equipment and platforms covered with dust, top cleaning required","Miscellaneous","General Appearance","Behaviour Based","10.29","Medium","","","Old Discarded/ Condemend pilot ladder stowed at the platforms removed & cleaning carried out. ","2020-08-23T23:59:35","","Completed","2020-07-30T23:59:35","No","No","No","Internal","job to be completed as planned and close out"]
[null,null,null,13264,null,"53_19/07/2020 14:57:31","2020-07-03T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Steering gear room pipe rack to fabricate.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","PIPE RACK FABRICATED.                                   JOB NO:V-DPUM028304/20","2020-08-23T23:59:35","","Completed","2020-07-25T23:59:35","No","No","No","Internal","job to be completed as planned and close out"]
[null,null,null,13265,null,"53_19/07/2020 15:11:40","2020-07-03T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Mooring winches several sight glass not clear and the oil colour shows sign of water content.","Deck - Machinery,Deck - Mooring Machinery","Mooring","Equipment Related,External Factors","11.4","Very High","","","Oil drained and flushing carried out. Gasket renewed for the inspection door. o ring replaced for the breather cap.Jobno-Vdpum 027857/20\n\nVdpum 027858/20\n\n","2020-08-23T23:59:35","","Completed","2020-07-30T23:59:35","No","No","No","Internal","job to be completed as planned and close out"]
[null,null,null,13266,null,"53_19/07/2020 15:13:14","2020-07-03T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Reducer on top of emer gen room and main deck to be derusted and moved to P midship locker.","Deck - Machinery","General Appearance","Equipment Related","11.4","Very High","","","Derusting & painting of spare manifold reducers completed. ","2020-09-23T23:59:35","","Completed","2020-09-19T23:59:35","No","No","No","Internal","job to be completed as planned and close out"]
[null,null,null,13267,null,"53_19/07/2020 15:16:35","2020-07-03T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","FW tank capacitance gauge not functional / erratic","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Gauge replaced with the new spare received.    Job no:V-DPUM028639/20","2020-08-23T23:59:35","DPUM200199","Completed","2020-09-19T23:59:35","No","No","No","Internal","spares processed for supply; complete and close out on receipt of spares"]
[null,null,null,13268,null,"53_31/07/2020 7:50:49 AM","2020-07-03T23:59:35","Observation","Owner / Marine / Tech. Suptd.","ISM Audit","Each Winch greasing points were highlighted by yellow colored paint but same were not numbered.","Deck - Mooring Machinery","Mooring","Behaviour Based,Inappropriate Procedure","9.13","Low","","","All mooring winch greasing points cleaned, Highlighted with yellow paint, same numbered & stencil in place.","2020-10-02T23:59:35","","Completed","2020-08-09T23:59:35","No","No","No","Internal"]
[null,null,null,13271,null,"53_19/07/2020 12:58:19","2020-07-03T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Crew laundry water dripping from sealing","Accommodation","General Appearance","Equipment Related","","","","","Pin hole leak from fresh water same rectified by cold repairs.","2020-07-23T23:59:35","","Completed","2020-07-09T23:59:35","No","No","No","Internal"]
[null,null,null,13272,null,"53_19/07/2020 12:52:46","2020-07-03T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Poop deck winch rope covers, two of them have heavy deposits of carbon or grease like substance. – to renew","Deck - Mooring Machinery","Mooring","Equipment Related,Inappropriate Procedure","11.4","Very High","","","2 number of canvas cover renewed for Poop deck winch rope.","2020-07-23T23:59:35","","Completed","2020-07-12T23:59:35","No","No","No","Internal"]
[null,null,null,13273,null,"53_19/07/2020 13:02:47","2020-07-03T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Sunken deck alleyway needs to be stripped and waxed and later cover with plastic. Already sign of discolouration.","Accommodation","General Appearance","Behaviour Based","10.29","Medium","","","Sunken deck alleyway cleaned, stripped , waxed & plastic cover renewed.","2020-07-13T23:59:35","","Completed","2020-07-13T23:59:35","No","No","No","Internal"]
[null,null,null,13274,null,"53_19/07/2020 15:15:02","2020-07-03T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Lights illumination is less due to direction of tubelight fitting","Miscellaneous","Emgcy. Systems","Equipment Related","10.29","Medium","","","light fixture need to be changed. (ALL FIXTURES NEEDS TO BE REPLACED.) WILL BE DONE IN NEXT BUDGET YEAR","2020-07-23T23:59:35","","Completed","2020-07-19T23:59:35","No","No","No","Internal"]
[null,null,null,13275,null,"53_19/07/2020 13:10:49","2020-07-03T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Some notices and posters stuck to the bulkhead in alley ways; this must stop. All the notices should be limited to noticeboard only.","Accommodation","General Appearance","Inappropriate Procedure","10.29","Medium","","","Cargo & Bunker MSDS were posted on bulkhead same re- arranged & posted on Notice board.","2020-07-11T23:59:35","","Completed","2020-07-11T23:59:35","No","No","No","Internal"]
[null,null,null,13276,null,"53_31/07/2020 7:53:53 AM","2020-07-03T23:59:35","Observation","Owner / Marine / Tech. Suptd.","ISPS Audit","Port anchor in use. Although hawse pipe cover was in place, same was not secured.\n\n\n\n","Deck - Mooring Machinery","Mooring","Behaviour Based,Human Error","7.15","High","","","New securing arrangemet made for securing of the Hawse pipe when anchor is in use, Same kept in Focsle store & stencilled.","2020-10-02T23:59:35","","Completed","2020-07-21T23:59:35","No","No","No","Internal"]
[null,null,null,13277,null,"53_31/07/2020 8:05:48 AM","2020-07-03T23:59:35","Defect,Observation","Owner / Marine / Tech. Suptd.","MLC Audit","1. One drier air filter found covered with lint.\n\n\n\n2. Possible leakage noted at blower as water droplets were noted.\n\n","Accommodation","MLC Related","Behaviour Based,Human Error","11.14","Medium","","","1.Crew Re-Briefed about the importance of cleaning the filter before using the Driers, Same been very frequently checked for compliance & found in order.                 2.Ships laundry panel opened up & leaking FW pipe repaired & leakage of water ceased, Job completed.                                                                          ","2020-10-02T23:59:35","","Completed","2020-07-09T23:59:35","No","No","No","Internal"]
[null,null,null,13278,null,"53_19/07/2020 15:09:32","2020-07-03T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Natural vents around accom steel screen requires cleaning","Accommodation","General Appearance","External Factors","11.4","Very High","","","Natural vent steel screen removed cleaned, derusted/ painted & put back in place.","2020-07-24T23:59:35","","Completed","2020-07-22T23:59:35","No","No","No","Internal"]
[null,null,null,13167,null,"53_15/07/2020 13:48:56","2020-07-08T23:59:35","Observation","Ship Staff","Ship Staff Insp.","AHU RECIRCULATION DUCTING HAS AN OPENING WITHOUT THE MANHOLE COVER. tHIS IS CAUSING WHSITLING SOUND IN ACCOMODATION B-DECK","Accommodation","MLC Related","Human Error,Industry Issue","","","","","PLATE FABRICATED AS MANHOLE COVER AND FITTED IN PLACE.","2020-07-13T23:59:35","","Completed","2020-07-14T23:59:35","No","No","No","Internal","kindly revert in separate mail, no changes to be made without office approval."]
[null,null,null,13479,null,"53_15/08/2020 1:30:21 PM","2020-07-10T23:59:35","Defect","Ship Staff","Ship Staff Insp.","PUMP ROOM FIXED GAS DETECTION O2 SENSOR FAULTY.","Miscellaneous","Cargo / Ballast Systems","Equipment Related","","","","","H2S and O2 detector with sensor replaced with new one and calibration carried out.Damaged Benzo connector renewed.                                   Job no:V-DPUM028641/20","2020-09-23T23:59:35","DPUM200196","Completed","2020-09-18T23:59:35","No","No","No","Internal","spares confirmed for supply awaiting connection"]
[null,null,null,13480,13480,"53_15/08/2020 1:27:23 PM","2020-07-13T23:59:35","Defect","Ship Staff","Ship Staff Insp.","NO 2 CARGO STRIP EDUCTOR SUCTION PRESSURE GAUGE, \tNO 2 CARGO STRIP EDUCTOR DRIVING PRESSURE NO 2 CARGO STRIP EDUCTOR DISCHARGE PRESSURE GAUGE ,VAPOUR COLLECTION MAIN PIPE PRESS GAUGE IN CCR FAULTY","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","10.32","Very High","","","NO.2 Cargo eductor Suction, discharge, drive & VECS gauge zero adjustment & callibration carried out same under observation.","2020-10-23T23:59:35","DPUM200200","Completed","2020-10-20T23:59:35","No","No","No","Internal","awaiting detailed feed back from ship"]
[null,null,null,13269,null,"53_27/07/2020 1:23:22 PM","2020-07-19T23:59:35","Defect","Ship Staff","Ship Staff Insp.","FWG CONTROLLER DEFECTIVE","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Defective controller replaced with the spare received and calibrated working satisfactory. Job no :V-DPUM028640/20","2020-09-15T23:59:35","DPUM200204","Completed","2020-09-18T23:59:35","No","No","No","Internal","processed for supply."]
[null,null,null,13270,null,"53_31/07/2020 12:28:13","2020-07-21T23:59:35","Defect","Ship Staff","Ship Staff Insp.","FWG   flowmeter not showing correct reading.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Spare received, job planned in upcoming week","2021-01-17T23:59:35","DPUM200206","Completed","2021-01-11T23:59:35","No","No","No","Internal","confirm if the spares rcd at Singapore- close out ASAP"]
[null,null,null,13481,null,"53_15/08/2020 1:06:06 PM","2020-07-31T23:59:35","Non Conformity","Ship Staff","Ship Staff Insp.","Pump room light fixture interlock switch not in place.","Elect. Mach. & Equip.","Emgcy. Systems","Equipment Related","11.11","Very High","","","Switch rcvd and replaced. Defect rectified and closed.","2020-10-30T23:59:35","DPUM200212","Completed","2020-09-19T23:59:35","No","No","No","Internal","spares arranged , kindly confirm if rcd. \nclose out the job once completed"]
[null,null,null,16535,null,"53_26/12/2020 7:09:13 PM","2020-08-01T23:59:35","Non Conformity","Ship Staff","Ship Staff Insp.","During the renewal of light in the pump room found one of the pump room light fixture is without interlock switch.","Elect. Mach. & Equip.","Cargo / Ballast Systems","Equipment Related,External Factors,Industry Issue","8.48","Medium","","","Vessel received this R.O at Singapore, Rectification completed. Light in order.","2020-10-31T23:59:35","DPUM200212 ","Completed","2020-09-19T23:59:35","No","No","No","Internal"]
[null,null,null,13482,null,"53_15/08/2020 1:12:12 PM","2020-08-05T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Smoke detector sensor in suez cabin detector fault alarm.","Elect. Mach. & Equip.,LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","replace with spare smoke detector sensor onboard.RO rasied for the same.","2020-08-08T23:59:35","DPUM200218","Completed","2020-08-05T23:59:35","No","No","No","Internal"]
[null,null,null,13939,null,"53_03/09/2020 1:41:59 AM","2020-08-08T23:59:35","Breakdown,Defect","Ship Staff","Ship Staff Insp.","Hydraulic hose of brake testing Kit for Mooring winch is parted.","Miscellaneous","Mooring","Equipment Related","9.7","Medium","","","spare received replaced the damage hose tried out working satisfactory.","2020-11-07T23:59:35","DPUM200168","Completed","2020-09-18T23:59:35","No","No","No","Internal"]
[null,null,null,13587,null,"53_20/08/2020 4:14:08 PM","2020-08-09T23:59:35","Breakdown,Defect","Ship Staff","Ship Staff Insp.","STBD WINDLASS BRAKE SEALS LEAKING, SAME NEEDS TO BE RENEWED.","Deck - Mooring Machinery","Mooring","Equipment Related","","","","","SEALS RENEWED AND WINDLASS TRIED OUT. NO LEAKAGES, ALL SATISFACTORY.                       JOB NO:V-DPUM028155/20","2020-08-24T23:59:35","","Completed","2020-08-12T23:59:35","No","No","No","Internal"]
[null,null,null,13588,null,"53_22/08/2020 09:13:13","2020-08-09T23:59:35","Defect","Ship Staff","Ship Staff Insp.","PORT  WINDLASS BRAKE SEALS LEAKING, SAME NEEDS TO BE RENEWED.","Deck - Mooring Machinery","Mooring","Equipment Related","","","","","SEALS RENEWED AND WINDLASS TRIED OUT. NO LEAKAGES, ALL SATISFACTORY.                       JOB NO:V-DPUM028156/20","2020-08-24T23:59:35","","Completed","2020-08-14T23:59:35","No","No","No","Internal"]
[null,null,null,13585,null,"53_31/08/2020 7:13:08 AM","2020-08-16T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Tape wiper assembly leaking for UTI.S.NO.6375","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.12","Medium","","","Spares recd. and renewed. UTI in good working condition.","2020-12-24T23:59:35","DPUM200222","Completed","2020-12-17T23:59:35","No","No","No","Internal","spares confirmed for supply"]
[null,null,null,13586,null,"53_28/08/2020 16:27:46","2020-08-21T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Composite boiler F.O solenoid valve non operational.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","New spare received was installed, now operational.","2020-10-31T23:59:35","DPUM200231","Completed","2020-11-07T23:59:35","No","No","No","Internal","Spares to be connected at US ( mid Nov)"]
[null,null,null,13589,null,"53_31/08/2020 11:42:29","2020-08-22T23:59:35","Defect","Ship Staff","Ship Staff Insp.","STBD HHC slewing pump bearing lubricating pot top cover badly rusted and corroded.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related,External Factors","","","","","Same repaired and top cover fabricated. Derusting carried out.","2020-08-24T23:59:35","","Completed","2020-08-23T23:59:35","No","No","No","Internal"]
[null,null,null,13940,null,"53_05/09/2020 9:16:13 AM","2020-08-26T23:59:35","Defect","Ship Staff","Ship Staff Insp.","UTI S.NO. 6454 -- Temperature is varying by 0.8 to 0.9 centigrade when compared with standard thermometer & other 2 onboard uti's and is also erratic.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.12","Medium","","","UTI S.NO. 6454 serviced & Repaired at singapore on 22 Sep 2020 & received back onboard with certificate. ","2020-11-24T23:59:35","DPUM200223","Completed","2020-09-15T23:59:35","No","No","No","Internal","Serv confirmed at Singapore on 21st Sept with BOND"]
[null,null,null,13942,null,"53_05/09/2020 8:46:18 AM","2020-08-27T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Section of VRCS return line found holed IWO manifold crossover valves.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.11","Medium","","","Section of pipeline from VRCS return line removed, welded in engine room workshop & put back in place. System tested & no leaks observed. Unplanned job carried out & Reported in PMS, Job order number V-DPUM028351/20","2020-08-31T23:59:35","","Completed","2020-08-27T23:59:35","No","No","No","Internal"]
[null,null,null,13943,null,"53_05/09/2020 9:02:48 AM","2020-08-28T23:59:35","Defect","Ship Staff","Ship Staff Insp.","IG line expansion coupling below No.5 Foam monitor platform leaking/ hissing noise from the joint.\t ","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.11","Medium","","","IG line Expansion coupling near No.5 Foam Monitor valve was opened up for inspection as same had a  hissing(passing) noise at joints.\n\nExpansion coupling opened cleaned/ inspected / lubricated & put back in service.No hissing noise found after completion of job.Unplanned job reported in PMS & completed, Job order Number V-DPUM 028357/20\n\n","2020-09-03T23:59:35","","Completed","2020-08-28T23:59:35","No","No","No","Internal"]
[null,null,null,14125,null,"53_19/09/2020 1:03:15 AM","2020-09-06T23:59:35","Breakdown,Non Conformity","Ship Staff","Mooring Audit","Parting of Aft Number 1 Inboard breast line mooring tail at Berth -Waidiao, port - Zhoushan, China. Mooring winch 7A.","Miscellaneous","Mooring","Equipment Related,External Factors","9.17","High","","","Broken mooring tail was renewed with the available spare new mooring tail & discharge operations resumed safely thereafter.Unplanned job reported in PMS & completed, Job order Number V-DPUM028567/20\n\n","2020-09-08T23:59:35","","Completed","2020-09-06T23:59:35","No","No","No","Internal"]
[null,null,null,13944,null,"53_14/09/2020 16:26:14","2020-09-06T23:59:35","Defect","Ship Staff","Ship Staff Insp.","HYDRAULIC VALVE VRC OT-114 NOT OPERATING.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","COIL INSPECTED FOUND BURNT.SAME RENWED WITH SPARE AVAILABLE ONBOARD.                  JOB NO:V-DPUM028351/20\n\n","2020-09-23T23:59:35","","Completed","2020-09-06T23:59:35","No","No","No","Internal"]
[null,null,null,16537,null,"53_26/12/2020 7:15:20 PM","2020-09-06T23:59:35","Non Conformity","Ship Staff","Ship Staff Insp.","Parting of Aft Number 1 Inboard breast line mooring tail at Berth -Waidiao, port - Zhoushan, China. Mooring winch 7A.","Deck - Mooring Machinery","Mooring","External Factors","9.17","High","","","Broken mooring tail was renewed with the available spare new mooring tail & discharge operations resumed safely thereafter. ","2020-11-05T23:59:35","","Completed","2020-09-11T23:59:35","No","No","No","Internal"]
[null,null,null,14126,null,"53_18/09/2020 17:23:44","2020-09-08T23:59:35","Defect","Ship Staff","Ship Staff Insp.","STEERING GEAR WATER FOUNTAIN LEAKING.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","REMOVED THE INSULATION LAGGING FOUND THE CRACK AT THE BOTTOM OF THE WATER CASING SAME REPAIRED CARRIED OUT BY BRAZING.   JOB NO:V-DPUM028566/20","2020-09-19T23:59:35","","Completed","2020-09-11T23:59:35","No","No","No","Internal"]
[null,null,null,13941,null,"53_15/09/2020 10:06:16 AM","2020-09-08T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Approximate 5 to 8% of the VRCS supply & Return line needs derusting/ Painting(Exposed section), & approximate 15 to 20% of the Support/ clamps need Derusting/painting & Re-insertion of new teflon sheet.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.11","Medium","","","All jobs under Superientendent Inspection Report dated 22 Sep 2020 have been added in DDRL, to avoid duplication of jobs, this item is removed from the pending list & monitored as per the updated DDRL.","2020-12-18T23:59:35","","Completed","2020-10-21T23:59:35","No","No","No","Internal","job to complete as planned and close out"]
[null,null,null,14113,null,"53_30/09/2020 4:11:55 AM","2020-09-15T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Pump room blower suction filter mesh to repair","Deck - Machinery","Cargo / Ballast Systems","Equipment Related","11.4","Very High","","","Pumproom blower suction wire mesh rrenewed and found in good order.","2020-12-14T23:59:35","DPUM200207","Completed","2020-12-14T23:59:35","No","No","No","Internal","stores re- supplied at Corpous Christe. kindly revert with status"]
[null,null,null,14114,null,"53_30/09/2020 4:17:35 AM","2020-09-15T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Deck hydraulic line Teflon to replace with 5 mm pieces","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","11.4","Very High","","","Derusting / Painting of deck VRCS line & insertion of teflon pieces is completed. Fwd mooring hydaulic lines from Forecastle to Fwd spring winch derusting/ painting & insertion of new teflon pieces completed.","2020-12-14T23:59:35","","Completed","2020-12-02T23:59:35","No","No","No","Internal","material supplied, job to be completed as planned."]
[null,null,null,14115,null,"53_30/09/2020 4:33:41 AM","2020-09-15T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Crew smoke room leonal flooring to repair. DD spec to raise","Accommodation","General Appearance","Equipment Related","10.29","Medium","","","Job added in DD spec (Refman) for permanent repairs.","2021-08-14T23:59:35","","Completed","2020-12-08T23:59:35","No","No","No","Internal","job to be added to refman and plan for the upcoming DD."]
[null,null,null,14116,null,"53_30/09/2020 4:43:04 AM","2020-09-15T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Forecastle davit, swirl gear mechanism to ease off and derusting/painting to be done","Deck - Machinery","General Appearance","Equipment Related","11.4","Very High","","","Derusting/ painting of complete Forecastle davit is completed & Swirl gear mechanism lubricated.","2020-11-14T23:59:35","","Completed","2020-10-20T23:59:35","No","No","No","Internal","complete and close out as planned."]
[null,null,null,14117,null,"53_30/09/2020 4:46:44 AM","2020-09-15T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Crew mess room chairs to clean. Plan cloth renewal at docking","Accommodation","General Appearance","Behaviour Based","10.29","Medium","","","Cleaning of crew mess room chairs carried out to best possible. (Unable to clean the fabric completely as cannot be removed and washed). Job added in Refman for renewal of cloth on chairs during DD. ","2021-08-14T23:59:35","","Completed","2020-12-08T23:59:35","No","No","No","Internal","plan cleaning or renewal during docking"]
[null,null,null,14118,null,"53_30/09/2020 4:51:07 AM","2020-09-15T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Forecastle store equipment and platforms covered with dust, top cleaning required","Miscellaneous","General Appearance","Behaviour Based","10.29","Medium","","","Cleaning of forecastle store equipment & platforms completed.","2020-11-14T23:59:35","","Completed","2020-10-07T23:59:35","No","No","No","Internal","complete and close out as planned."]
[null,null,null,14119,null,"53_30/09/2020 4:54:07 AM","2020-09-15T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Port Hose handling crane to be planned for cleaning and painting","Cargo Mach.","General Appearance","Equipment Related","10.29","Medium","","","Cleaning of Port Hose handling crane carried out.","2020-11-14T23:59:35","","Completed","2020-10-24T23:59:35","No","No","No","Internal","complete as planned"]
[null,null,null,14121,null,"53_30/09/2020 5:05:12 AM","2020-09-15T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Stbd bunker tank vend head corroded flap facing forward to renew","Deck - Machinery","General Appearance","Equipment Related","11.4","Very High","","","Stbd side Bunker tank vent head corroded section renewed, painted & put back in place.","2020-10-14T23:59:35","","Completed","2020-10-07T23:59:35","No","No","No","Internal","complete and close out as planned."]
[null,null,null,14122,null,"53_30/09/2020 5:02:18 AM","2020-09-15T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Accom AC filter corroded, to renew","Deck - Machinery","General Appearance","Equipment Related","11.4","Very High","","","filters received and replaced","2021-01-23T23:59:35","DPUM200287","Completed","2021-01-04T23:59:35","No","No","No","Internal","prefab filters supplied passing Singapore"]
[null,null,null,14123,null,"53_30/09/2020 5:15:24 AM","2020-09-15T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Hyd Crane operator protection covers to be fabricated for all the cranes","Cargo Mach.","Safety / LSA / FFA","Behaviour Based,Equipment Related","8.5","Very High","","","Protection covers for P & S HHC  // P & S Provision crane fabricated / painted & put in place.JOB NO:V-DPUM028997/20, V-DPUM028794/20","2020-10-14T23:59:35","","Completed","2020-10-03T23:59:35","No","No","No","Internal","complete and close out as planned."]
[null,null,null,14124,null,"53_30/09/2020 5:26:22 AM","2020-09-15T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Spare stand for ME liner pending for fabrication","Miscellaneous","General Appearance","Equipment Related","10.29","Medium","","","M.E SPARE LINER STAND FABRICATED  AND INSTALLED IN PLACE.\n\nJOB NO:V-DPUM028996/20","2020-11-14T23:59:35","","Completed","2020-10-01T23:59:35","No","No","No","Internal","complete and close out as planned."]
[null,null,null,14127,null,"53_30/09/2020 4:37:55 AM","2020-09-15T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Both life boat davit hinge pins to free up; as they are observed to be moving with the davit now","LSA / FFA","Safety / LSA / FFA","Equipment Related","10.29","Medium","","","P & S Lifeboat davit hinge pins inspected on 26 Sep 2020 during weekly Lifeboat drills & found in order. Davit pins are in place & are not moving when Lifeboat is moved from its stowed position.","2020-10-08T23:59:35","","Completed","2020-09-19T23:59:35","No","No","No","Internal"]
[null,null,null,14128,null,"53_30/09/2020 5:24:30 AM","2020-09-15T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Some major spares in ER need stencilling or tagging with readable laminations","Miscellaneous","General Appearance","Behaviour Based","10.29","Medium","",""," Laminated tag on all the major spares in ER put in place","2020-09-23T23:59:35","","Completed","2020-09-20T23:59:35","No","No","No","Internal"]
[null,null,null,14129,null,"53_30/09/2020 5:46:27 AM","2020-09-15T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Steering gear radiator annual cleaning – change request to forward","Miscellaneous","Eng. / Strg. Comp.","Human Error","","","","","CRF send to office for approval","2020-09-22T23:59:35","","Completed","2020-09-20T23:59:35","No","No","No","Internal"]
[null,null,null,14130,null,"53_30/09/2020 5:50:35 AM","2020-09-15T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Several Spare ME fuel valves not ready for use","Miscellaneous","Eng. / Strg. Comp.","Behaviour Based","10.29","Medium","","","All the spare fuel valve overhauled and pressure tested and kept ready for use.","2020-09-23T23:59:35","","Completed","2020-09-19T23:59:35","No","No","No","Internal"]
[null,null,null,14131,null,"53_30/09/2020 12:48:02","2020-09-15T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Spare ME piston rod slight sign of corrosion. Piston rod to be oiled","E/R - Main Engine","Eng. / Strg. Comp.","External Factors","","","","","Piston rod cleaned and oiled and wrapped with plastic sheet.","2020-09-23T23:59:35","","Completed","2020-09-19T23:59:35","No","No","No","Internal"]
[null,null,null,14132,null,"53_30/09/2020 5:43:31 AM","2020-09-15T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Boiler 3M job change request to include water level blowdown, air transmitter lines cleaning and exercise the solenoid valves to be send","Miscellaneous","Eng. / Strg. Comp.","Human Error","","","","","CRF Send to office for approval","2020-10-14T23:59:35","","Completed","2020-09-23T23:59:35","No","No","No","Internal"]
[null,null,null,14133,null,"53_30/09/2020 5:08:43 AM","2020-09-15T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","One winch stbd fwd, minor leak from control lever to rectify","Deck - Machinery","Mooring","Equipment Related","11.4","Very High","","","Union connection to isolating valve found loose tightened the same.","2020-09-23T23:59:35","","Completed","2020-09-21T23:59:35","No","No","No","Internal"]
[null,null,null,14464,null,"53_24/10/2020 3:00:20 PM","2020-09-15T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Cargo Audit","Ship/shore safety check list remarks column for smoking area and Naked light not filled with adequate information\n\n\n\n","Miscellaneous","Cert. & Docu.","Human Error","5.9","Very High","","","Smoking area & naked light regulation comes under Part 5A & Part 6 of SSSCL, Part 6 was duly filled, In part 5A reference has been made to refer to Part 6.","2020-09-23T23:59:35","","Completed","2020-09-16T23:59:35","No","No","No","Internal"]
[null,null,null,14465,null,"53_24/10/2020 3:03:55 PM","2020-09-15T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Mooring Audit","Last annual BHC test was conducted on 15 Aug 2019 which is due on 15 Aug 2020. \n\n","Miscellaneous","Mooring","Equipment Related,External Factors,Human Error","9.7","Medium","","","Annual BHC test conducted for all mooring winches on 25 Sep 2020, after receipt of hydraulic hose for winch brake testing pump.","2020-09-23T23:59:35","","Completed","2020-09-18T23:59:35","No","No","No","Internal"]
[null,null,null,14466,null,"53_24/10/2020 3:09:58 PM","2020-09-15T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Nav Audit / Verification","Auto pilot operation on transmitting magnetic compass tested everyday, however, no record was sighted available. \n\n","Documentation,Navigation - Others","Navigation","Human Error","4.3","Medium","","","After testing of Auto pilot on TMC mode deck logbook entry made.","2020-09-23T23:59:35","","Completed","2020-09-19T23:59:35","No","No","No","Internal"]
[null,null,null,16538,null,"53_26/12/2020 8:38:12 PM","2020-09-15T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Ship/shore safety check list remarks column for smoking area and Naked light not filled with adequate information","Documentation","Cert. & Docu.","Human Error","5.9","Very High","","","Smoking area & naked light regulation comes under Part 5A & Part 6 of SSSCL, Part 6 was duly filled, In part 5A reference has been made to refer to Part 6.","2020-10-24T23:59:35","","Completed","2020-09-16T23:59:35","No","No","No","Internal"]
[null,null,null,16539,null,"53_26/12/2020 8:46:41 PM","2020-09-15T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Last annual BHC test was conducted on 15 Aug 2019 which is due on 15 Aug 2020. ","Deck - Mooring Machinery","Mooring","Equipment Related","9.7","Medium","","","Annual BHC test conducted for all mooring winches on 25 Sep 2020, after receipt of hydraulic hose for winch brake testing pump.","2020-10-24T23:59:35","","Completed","2020-09-18T23:59:35","No","No","No","Internal"]
[null,null,null,14467,null,"53_17/10/2020 4:42:49 PM","2020-10-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","IG Branch valve Spindle Bush found Cracked for 1C, 1P, 1S, 2C, 4S, 5P, 5S & Slp P COT.\t","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.11","Medium","","","Spindle bush for IG branch valve to be fabricated as per sample at 1st available opportunity in port by shore vendor.","2020-10-31T23:59:35","","Completed","2020-10-13T23:59:35","No","No","No","Internal"]
[null,null,null,14468,null,"53_28/10/2020 3:27:13 PM","2020-10-16T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","Forward Hydraulics -- Section of cooling water inlet line leaking with pin hole\n\n","Deck - Mooring Machinery,Deck - Pipe / Fittings","General Appearance","Equipment Related","11.4","Very High","","","Section of pipe removed, Repaired & put back in place; Job Order No.--- V-DPUM029229/20","2020-10-18T23:59:35","","Completed","2020-10-16T23:59:35","No","No","No","Internal"]
[null,null,null,14469,null,"53_25/10/2020 10:26:45 AM","2020-10-17T23:59:35","Defect","Ship Staff","Ship Staff Insp.","STBD LIFEBOAT SEARCH LIGHT SWITCH DEFECTIVE.","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.29","High","","","SEARCH LIGHT SWITCH REPAIRED. RO RAISED FOR SEARCH LIGHT","2020-11-23T23:59:35","DPUM200292","Completed","2020-10-21T23:59:35","No","No","No","Internal"]
[null,null,null,12852,null,"53_23/06/2020 6:27:38 AM","2020-10-22T23:59:35","Defect","Ship Staff","Ship Staff Insp.","During Routine inspection found that cargo sampling device has kinks on the tape.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.12","Medium","","","Vessel does not have any spare tape for cargo sampling device. PO raised for the same awaiting spares.","2021-01-24T23:59:35","DPUM200156","Completed","2021-02-09T23:59:35","No","No","No","Internal","spares connected and close out"]
[null,null,null,15860,null,"53_08/12/2020 5:59:06 PM","2020-10-26T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Stbd crane high pressure hydraulic line has very small leak","Deck - Machinery","Structural Condn. / WT integrity ","Equipment Related","8.5","Very High","","","Crane was operated in presence of CO, Bosun, 2E to find any visible leaks, found none.","2020-12-24T23:59:35","","Completed","2020-11-13T23:59:35","No","No","No","Internal"]
[null,null,null,15449,null,"53_03/12/2020 07:57:26","2020-11-10T23:59:35","Breakdown","Ship Staff","Engineering Audit","HFO Purifier bowl leaking","E/R - Purifier","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Purifier is operational and in service now. Below trouble shooting were carried out- centrifugal clutch was overhauled, inlet pipe pairing tube washers were renewed.Assembly rechecked as per instruction manual.","2020-11-28T23:59:35","","Completed","2020-11-24T23:59:35","No","No","No","Internal","issue resolved as per mail , under monitoring ; close out once all good."]
[null,null,null,15861,null,"53_08/12/2020 6:13:17 PM","2020-11-16T23:59:35","Other","Ship Staff","Ship Staff Insp.","Cross over valve for No-2 line and 3 valves of Marpol line valve found freeze and required O’hauling.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.11","Medium","","","Overhauling carried out for the same.","2020-11-23T23:59:35","","Completed","2020-11-20T23:59:35","No","No","No","Internal"]
[null,null,null,15862,null,"53_15/12/2020 10:50:11 AM","2020-12-01T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Forward windlass anchor chain stopper gratings and supports found rusted. Same to be upgraded cosmetically.","Deck - Mooring Machinery","Mooring","Equipment Related","9.14","Medium","","","Forward windlass gratings and supports chipped, buffed and painted. ","2020-12-18T23:59:35","","Completed","2020-12-08T23:59:35","No","No","No","Internal"]
[null,null,null,15858,null,"53_11/12/2020 10:36:38","2020-12-03T23:59:35","Defect","Ship Staff","Ship Staff Insp.","AC Compressor no.2, stage 3 stbd unit oil scraper ring, suction plate broken","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Compressor all 3 stages were opened up for inspection and trouble shooting, below were the findings stage wise- No.1 stage- dischage plate broken for one of the unit, which was renewed. Rocker arm assembly intact. Liner & piston unit found intact with no score marks. No.2 Unit- Found score marks on piston crown top land, suction plate broken for one of the unit. Rocker arm assembly found dislodged from the pivot with one of the spring clamp broken, both liners were overhalued with new suction plate and springs. Dischage valve plate was renewed for both units with new gaskets. No.3 stage- Both units liners were overhauled with new suction plate and new o rings and gaskets. stbd unit piston renewed with complete new piston with rings. Compressor unloading unit- rocker arm fucntion checked for all units, operating satisfactory. Compressor Oil refilled and checked for any leaks. No leaks. Compressor tested on load with all 3 stages, working perfectly fine.","2021-01-08T23:59:35","DPUM200304","Completed","2021-01-02T23:59:35","No","No","No","Internal","spares connected at Singapore; revert with the plans for OH"]
[null,null,null,15859,null,"53_15/12/2020 10:38:25 AM","2020-12-03T23:59:35","Observation","Ship Staff","Ship Staff Insp.","15 nos. COW machine and isolation valves found hard to operate.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.34","High","","","All COW machine and isolation valves freed up and overhauled and are well lubricated to ensure free and smooth operation .","2020-12-24T23:59:35","","Completed","2020-12-12T23:59:35","No","No","No","Internal","complete as planned and close out"]
[null,null,null,16523,null,"53_30/12/2020 10:07:45","2020-12-11T23:59:35","Defect,Observation","Ship Staff","Ship Staff Insp.","Crew mess room A/C duct condenstion leak","Accommodation","General Appearance","Equipment Related","10.32","Very High","","","Defect has been put in refman for  drydocking repir","2021-01-30T23:59:35","","Completed","2021-02-21T23:59:35","No","No","No","Internal","completed at yard"]
[null,null,null,16540,null,"53_31/12/2020 8:42:12 PM","2020-12-16T23:59:35","Observation","Ship Staff","Ship Staff Insp.","3 nos. cargo tanks I.G. inlet valve found hard to operate.","Inert Gas","Cargo / Ballast Systems","Equipment Related","8.2","Medium","","","All three I.G. inlet valves worm gear assembly was opened up and overhauled. Greasing done of the valves and boxed back. All operating smoothly.","2020-12-24T23:59:35","","Completed","2020-12-21T23:59:35","No","No","No","Internal"]
[null,null,null,15857,null,"53_08/12/2020 6:09:53 PM","2020-12-22T23:59:35","Observation","Ship Staff","Ship Staff Insp.","No-2 separator is indicating oil in separator","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.8","Medium","","","Separator showing correct readings after tank cleaning and discharging operations in Yosu. Calibration done by HKT marine in drydock. All found satisfactory. Defect closed out.","2021-03-07T23:59:35","","Completed","2021-01-30T23:59:35","No","No","No","Internal","complete as planned and close out.\nrevert in separate mail in unable to resolve, for expert advise"]
[null,null,null,14112,null,"53_16/09/2020 15:53:16","2020-12-23T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","BWTS Filteration unit backflush line orfice to install.","Cargo Mach.","Cargo / Ballast Systems","Industry Issue","","","","","To install orfice on the backflushing system once recieved please refer the mail for installation.","2021-01-24T23:59:35","","Completed","2021-02-21T23:59:35","No","No","No","Internal","orifice plate rcd and fitted"]
[null,null,null,16525,null,"53_31/12/2020 8:48:54 PM","2020-12-24T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Walkway ramps on deck have their angle support bar plates thinned down in quite a few locations.","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","External Factors","11.5","Medium","","","Total no. of of angle supports, which are thinned down to be checked and same to be entered in the dry-dock specs via Refman.","2021-02-08T23:59:35","DPUM200207","Completed","2021-02-21T23:59:35","Yes","No","No","Internal","completed"]
[null,null,null,14462,null,"53_30/10/2020 08:33:53","2020-12-25T23:59:35","Observation","Ship Staff","Ship Staff Insp.","M3 Mooring winch directional control valve control lever slight leak.","Deck - Mooring Machinery","Mooring","Equipment Related","11.4","Very High","","","To renew the o-rings.Vessel has raised the RO for the same.","2021-01-21T23:59:35","DPUM200295","Completed","2021-02-21T23:59:35","No","No","No","Internal","spares received & rectified"]
[null,null,null,18276,null,"53_15/03/2021 1:48:33 PM","2021-01-05T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Aft Fire Wire reel not turning on load.","Deck - Mooring Machinery","Mooring","Equipment Related","9.17","High","","","Fire wire coil unspooled from drum. Alignment between the chain coupling and the reduction gear verified and boxed back the drum in place. Wire coiled back and tried out on load. Found working satisfactorily. ","2021-03-24T23:59:35","","Completed","2021-03-06T23:59:35","No","No","No","Internal"]
[null,null,null,16524,null,"53_30/12/2020 09:50:50","2021-01-28T23:59:35","Defect","Ship Staff","Ship Staff Insp.","ME FO auto backwash filter differential pressure transmitter faulty","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","ME FO autobackwash filter cleaned, DP pressure is not rising, Filter operation seems satisfactory","2021-05-01T23:59:35","DPUM210040","Completed","2021-05-11T23:59:35","No","No","No","Internal","spares processed for supply awaiting readyness"]
[null,null,null,18274,null,"53_13/03/2021 6:23:54 PM","2021-03-06T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Pumproom gas detection system showing flow fault on sample line no.2","Critical Equip.","Cargo / Ballast Systems","Equipment Related","8.46","Very High","","","All four sampling points were blown through to clear any residual moisture content. Sytem tried out and working satisfactorily. ","2021-03-21T23:59:35","","Completed","2021-03-11T23:59:35","No","No","No","Internal","complete as planned and close out"]
[null,null,null,18275,null,"53_13/03/2021 6:38:07 PM","2021-03-06T23:59:35","Defect","Ship Staff","Ship Staff Insp.","WBT gas detection system showing analyse pump / internal leakage fault.","Critical Equip.","Cargo / Ballast Systems","Equipment Related","5.21","Medium","","","Vacuum Switch No. 2 replaced of WBT gas detection system. Sytstem tried out and found working satisfatorily.","2021-03-15T23:59:35","","Completed","2021-03-12T23:59:35","No","No","No","Internal","revert if any shpre assistance or spares reqd / complete as planned."]
[null,null,null,18461,null,"53_30/03/2021 17:56:35","2021-03-22T23:59:35","Defect,Observation","Ship Staff","Ship Staff Insp.","Incinerator sluice door solenoid valve leaking","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","to order new soenoid valve and replace the exhisting solenoid","2021-05-03T23:59:35","","Completed","2021-08-24T23:59:35","No","No","No","Internal","key in the RO on priority for processing spares"]
[null,null,null,18462,null,"53_02/04/2021 13:13:57","2021-03-23T23:59:35","Defect,Observation","Ship Staff","Ship Staff Insp.","FWD Mast Steering light dimmer switch in W/H BCC panel defective.","Navigation - Others","Navigation","Equipment Related","4.8","Medium","","","RO-DPUM210014, Ordered new spare and same to replace once received.","2021-05-13T23:59:35","","Completed","2021-08-10T23:59:35","No","No","No","Internal","spares to be processed , once the quotes are received in system"]
[null,null,null,18463,null,"53_03/04/2021 21:55:27","2021-03-25T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Messman cabin toilet vaccum control mechanism was defetive, same was swapped from sunken deck toilet","Accommodation","MLC Related","Equipment Related","10.32","Very High","","","Require Vaccum control mechanim for sunken deck toilet to make it operational","2021-06-22T23:59:35","DPUM210047","Completed","2021-07-05T23:59:35","No","No","No","Internal","complete as planned upon receipt of spares."]
[null,null,null,19027,null,"53_1/5/2021 8:38:33 AM","2021-04-09T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Refrigerant Leak alarm sensor near Refrigeration Compressor not working.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Replace with new sensor upon recept of new spare. NEW SENSOR FITTED.","2021-05-25T23:59:35","DPUM210008","Completed","2021-06-07T23:59:35","No","No","No","Internal","spares confirmed for supply, check with procure and remind them for supply at the next convenient port."]
[null,null,null,19028,null,"53_01/05/2021 08:18:00","2021-04-13T23:59:35","Defect","Ship Staff","Ship Staff Insp.","UV sterilizer under current relay not working","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","To replace the relay upon receipt of spare. RELAY REPLACED WITH NEW SPARE.","2021-05-24T23:59:35","DPUM210037","Completed","2021-05-31T23:59:35","No","No","No","Internal","complete as planned upon receipt of spares. Follow up with procure for spares arrangements"]
[null,null,null,19029,null,"53_30/04/2021 15:36:46","2021-04-23T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Inside workshop welding area curtain height is insufficient and clerance from the floor is high","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","New curtain with proper height ordered and will be replace when received. CURTAIN RENEWED.","2021-05-18T23:59:35","DPUM210050","Completed","2021-06-01T23:59:35","No","No","No","Internal","RO processed as per mentioned.\nreplace the curtains on receipt and close out"]
[null,null,null,19488,null,"53_15/05/2021 10:08:46","2021-05-02T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Engine room overhead crane travelling and traversing motion wire insulation damaged.","E/R - Aux. Mach.,Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Requisition raised for new cables. Damaged cables to replace once received new cables. Damaged cables renewed.","2021-06-23T23:59:35","DPUM210067","Completed","2021-10-11T23:59:35","No","No","No","Internal","RO to be finalized soon for supply"]
[null,null,null,19489,null,"53_15/05/2021 09:45:36","2021-05-06T23:59:35","Breakdown,Defect","Ship Staff","Ship Staff Insp.","BWTS No.2 Electrolyzer SW feed pump leaking from mechanical seal","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","To overhaul the SW feed pump with new mechanical seal upon receipt of spares. RECEIVED THE SPARES. Overhauled the pump. Mechanical seal renewed.","2021-06-06T23:59:35","DPUM210083","Completed","2021-10-04T23:59:35","No","No","No","Internal","please mention the PO number for reference and processing spares."]
[null,null,null,19623,null,"53_30/05/2021 11:57:16 AM","2021-05-17T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Main deck structures, branch valves, cable trays require de-rusting and painting. Main deck requires a full recoat after structures have been attended to. \n\nFwd. of manifold - walkway bridges on main-deck, Mooring winches, Tank domes, Butterworth pockets, PV Valve pipe and supports to be cosmetically upgraded.\n\n","Deck - Machinery,Deck - Pipe / Fittings","General Appearance","External Factors","","","","","MAIN DECK FULL COAT PAINTING COMPLETED.","2021-12-24T23:59:35","","Completed","2021-10-23T23:59:35","No","No","No","Internal","work in progress ; pipe fitting and structures pending"]
[null,null,null,19626,null,"53_30/05/2021 12:00:31 PM","2021-05-17T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Markings on forward area of the main deck are fading out - to be renewed.","Miscellaneous","Safety / LSA / FFA","Human Error","","","","","Markings carried out.","2021-08-24T23:59:35","","Completed","2021-06-21T23:59:35","No","No","No","Internal","complete and close out as planned"]
[null,null,null,19627,null,"53_30/05/2021 12:05:48 PM","2021-05-17T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Photographic evidence of cleaning of filters and electrolysis plates of BWTS to be sent to office.","Cargo Mach.","Cargo / Ballast Systems","Human Error","","","","","Pictures to be forward to officer for records","2021-06-23T23:59:35","","Completed","2021-06-23T23:59:35","No","No","No","Internal","complete and close out as planned"]
[null,null,null,19629,null,"53_30/05/2021 12:07:40 PM","2021-05-17T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Anchor marking buoy missing","Deck - Mooring Machinery","Mooring","Human Error","","","","","Requisition  raised. Spare received.","2021-08-24T23:59:35","DPUM210101","Completed","2021-07-27T23:59:35","No","No","No","Internal","raise RO on priority\ncomplete and close out as planned"]
[null,null,null,19630,null,"53_03/06/2021 13:33:05","2021-05-17T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Steering gear tank spare charge tank to be topped up to minimum requirement","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Topped up the steering gear spare tank to the required minimum level. ","2021-05-23T23:59:35","","Completed","2021-05-21T23:59:35","No","No","No","Internal"]
[null,null,null,19631,null,"53_03/06/2021 13:36:31","2021-05-17T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Poster for cleaning of GE FO Flowmeter filter to be updated","Miscellaneous","Eng. / Strg. Comp.","Human Error","10.32","Very High","","","Updated the date for cleaning of the last flowmeter filter","2021-05-21T23:59:35","","Completed","2021-05-21T23:59:35","No","No","No","Internal"]
[null,null,null,19632,null,"53_08/06/2021 3:24:40 PM","2021-05-27T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","General housekeeping of deck stores including paint locker to be improved.","Miscellaneous","General Appearance","External Factors","","","","","All deck stores including paint locker re-arranged and cleaned.","2021-06-03T23:59:35","","Completed","2021-05-29T23:59:35","No","No","No","Internal"]
[null,null,null,19633,null,"53_08/06/2021 2:38:32 PM","2021-05-28T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Port Crane Wire found twisted near block.","Deck - Machinery","Safety / LSA / FFA","Equipment Related","","","","","Twist of crane wire removed.","2021-06-03T23:59:35","","Completed","2021-05-29T23:59:35","No","No","No","Internal"]
[null,null,null,19634,null,"53_08/06/2021 3:21:56 PM","2021-05-28T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Lock of IG branch valves to be put in place.","Miscellaneous","Cargo / Ballast Systems","Equipment Related","","","","","All IG branch valves locks put in place.","2021-06-03T23:59:35","","Completed","2021-05-29T23:59:35","No","No","No","Internal"]
[null,null,null,19628,null,"53_08/06/2021 3:38:16 PM","2021-05-29T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Spare wires for each crane to be clearly tagged to indicate the crane they are meant to be used on.","Deck - Machinery","General Appearance","Industry Issue","","","","","Tagging of spare wires carried out.","2021-06-23T23:59:35","","Completed","2021-06-19T23:59:35","No","No","No","Internal","complete and close out as mentioned"]
[null,null,null,19624,null,"53_03/06/2021 09:11:51","2021-05-30T23:59:35","Observation","Ship Staff","Engineering Audit","CCU3 Electrical noice detected alarm active.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","CCU connector opened, cleaned properly and connected back. Electrical noise found zero. ","2021-10-24T23:59:35","","Completed","2021-10-14T23:59:35","No","No","No","Internal","followup with Mr Solanki and fleet3 in separate mail. awaiting from last update"]
[null,null,null,19732,null,"53_16/06/2021 2:31:45 PM","2021-06-01T23:59:35","Observation","Ship Staff","Engineering Audit","AC to be put 60- 70% fresh airrecirculation to maintain a positive pressure in the accomodation.","Miscellaneous","MLC Related","Equipment Related","","","","","Air intake flapes buffed and cleaned. Evaporator chemically cleaned. El expansion valve setting to be verified with the maker.","2021-08-24T23:59:35","DPUM210097","Completed","2021-07-04T23:59:35","No","No","No","Internal","troubleshooting in progress; to be resolved soon.\nshore serv also arranged mid July at Singapore"]
[null,null,null,19625,null,"53_08/06/2021 3:08:49 PM","2021-06-01T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Port Side draft Gauge found showing eratic reading.","Miscellaneous","Cargo / Ballast Systems","Equipment Related","","","","","Zero and span calibration carried out of P/I Converter, tested and forund satisfactory.","2021-08-24T23:59:35","DPUM210176","Completed","2021-10-02T23:59:35","No","No","No","Internal","awaiting troubleshooting... follow up in separate mail with work done on the system"]
[null,null,null,19731,null,"53_16/06/2021 2:37:49 PM","2021-06-06T23:59:35","Breakdown","Ship Staff","Engineering Audit","ME LO auto back wash filter elemets found damaged and broken mesh found carried to the engine. Reason for the damage to be analysed to prevent furtherengine  damage.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","New set of elements received and fitted.System found working satisfactorily.","2021-09-01T23:59:35","","Completed","2021-10-03T23:59:35","No","No","No","Internal","complete filter cartridge  under bulk purchase; \nlead time of few months. we still have old usable spares if need arises. Kindly follow up with Procure 3 for possible connection in Nov."]
[null,null,null,19848,null,"53_21/06/2021 3:27:25 PM","2021-06-14T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Accomodation water observed to be discoloured at times(Quite Reddish),Samples taken by Shipstaff from Fresh water tanks found to be cleaned.Last Tanks Inspected/Cleaned Feb-21.","Miscellaneous","MLC Related","External Factors","","","","","Both Fresh water tanks samples taken found to be cleaned also tanks overflowed during the voyage. Under observation. FW tanks inspected. Hydrophore and line filter cleaned. suspect water discoloration is due turbulance takes place when air enter in to water outlet. Correct level of water in the hydrophore to be maintained.","2021-09-13T23:59:35","","Completed","2021-07-21T23:59:35","No","No","No","Internal","carry out hydrophore and mineralizer unit cleaning and once done; consider use of rust stabilizer from Unitor"]
[null,null,null,19849,null,"53_21/06/2021 3:34:50 PM","2021-06-14T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Crew Mess Room Water dripping from Overhead panel at times due to aircon condensation.","Accommodation","Structural Condn. / WT integrity ","External Factors","","","","","Insulation sheet put on the air duct and trunking. ","2021-09-13T23:59:35","DPUM210112","Completed","2021-07-08T23:59:35","No","No","No","Internal","it was discussed and vessel to install insulating material on the AC ducts. complete and close out as planned."]
[null,null,null,19850,null,"53_21/06/2021 5:11:34 PM","2021-06-14T23:59:35","Observation","Ship Staff","Ship Staff Insp.","CCR various gauges/Cargo eductor/Ballast eductor showing erratic readings.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","CCR various gauges, Cargo eductor & Ballast eductors calibrated.","2021-09-13T23:59:35","","Completed","2021-07-08T23:59:35","No","No","No","Internal","revert in separate mail to tech with the jobs done and follow up,  try remote troubleshooting first before we confirm the shore service."]
[null,null,null,19851,null,"53_21/06/2021 5:07:36 PM","2021-06-14T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Forward Fire hose box noticed to be damaged. ","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","Damaged fire hose box replaced with spare fire hose box.","2021-06-23T23:59:35","","Completed","2021-06-18T23:59:35","No","No","No","Internal"]
[null,null,null,20082,null,"53_04/07/2021 10:18:22","2021-06-26T23:59:35","Defect","Ship Staff","Engineering Audit","Emergency generator Radiator tube leaking.","Elect. Mach. & Equip.","Emgcy. Systems","Equipment Related","","","","","Renew the radiator. Renewed the radiator","2021-10-24T23:59:35","DPUM210116","Completed","2021-10-02T23:59:35","No","No","No","Internal","Spares processed for supply. awaiting connection arrangements"]
[null,null,null,20081,null,"53_13/07/2021 12:05:00","2021-06-29T23:59:35","Observation","Ship Staff","Engineering Audit","AE fuel viscometer reading is erratic.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","Planning to dismantle the viscometer probe / clean and investigate. SENSOR CLEANED.","2021-07-24T23:59:35","","Completed","2021-07-12T23:59:35","No","No","No","Internal","complete as planned and close out. Serv RO will be required for shore assistance if required."]
[null,null,null,20230,null,"53_27/07/2021 11:34:50 AM","2021-07-03T23:59:35","Observation","Ship Staff","Engineering Audit","Frequent alarm from ME BWMS on the AMS and to save alarm printer cartridge and paper if alarm hystory printed, alarms are kept off scanned.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Configuration carried out as per maker's advise. System found satisfactory.","2021-12-24T23:59:35","","Completed","2021-10-01T23:59:35","No","No","No","Internal"]
[null,null,null,23314,null,"53_01/11/2021 9:33:46 PM","2021-07-03T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Cover for Waste oil tank to renew","Hull & Tanks","General Appearance","Equipment Related","6.9","Low","","","Tank vent cover cover and wire mesh renewed.","2021-08-23T23:59:35","","Completed","2021-08-23T23:59:35","No","No","No","Internal"]
[null,null,null,23315,null,"53_01/11/2021 9:39:29 PM","2021-07-03T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ME HPS System electric start up pump is unable to change over from MOP to select as master.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","MOP rebooted one by one and found start up pump selection and start functioning.","2021-10-24T23:59:35","","Completed","2021-10-03T23:59:35","No","No","No","Internal"]
[null,null,null,23316,null,"53_01/11/2021 9:43:28 PM","2021-07-03T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","To fabricate/ repair two air intake filter flaps for AC air handling unit.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Fabricated intake filters and fitted","2021-08-24T23:59:35","","Completed","2021-07-29T23:59:35","No","No","No","Internal"]
[null,null,null,20083,null,"53_15/07/2021 9:50:26 AM","2021-07-03T23:59:35","Observation","Ship Staff","Engineering Audit","Unable to change overr ( Select as master) the ME HPS electric start up pump from MOP","Elect. Mach. & Equip.,Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","Communication with electric automation department in progress. Received instruction from MAN B&W to reboot ECUs to resolve the issue. Waiting for suitable opportunity in a safe anchorage, port to reboot t the ECUs. Solved.","2021-09-23T23:59:35","","Completed","2021-07-29T23:59:35","No","No","No","Internal","please follow up in separate mail trail untill resolved"]
[null,null,null,20084,null,"53_13/07/2021 10:34:00 AM","2021-07-04T23:59:35","Defect","Ship Staff","Ship Staff Insp.","ODME flowmeter bypass valve spindle found stuck.","Cargo Mach.","MARPOL Related","Equipment Related","","","","","ODME flowmeter bypass valve spindle freed.","2021-08-08T23:59:35","","Completed","2021-07-24T23:59:35","No","No","No","Internal","close out as planned, reduced close out date to 15 Aug.\nsimple job - should not take that long"]
[null,null,null,26807,null,"53_Fri Sep 16 2022 03:26:50 GMT+0000","2021-07-05T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","M/E Bearing wear monitoring system gives frequent alarms due to faulty sensor","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Sensors are renewed by ship staff and KONGSEBERG attended with upgraded software.","2022-09-23T23:59:35","DPUM220177","Completed","2022-09-02T23:59:35","No","No","No","Internal"]
[null,null,null,20231,null,"53_29/07/2021 2:02:34 PM","2021-07-09T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Denso Tape of Hose handling Cranes to be renewed.","Deck - Machinery","Safety / LSA / FFA","Equipment Related","8.5","Very High","","","Denso Tape of Hose handling Cranes renewed.","2021-08-25T23:59:35","","Completed","2021-08-12T23:59:35","No","No","No","Internal","spares supplied last call Singapore; job should be completed on priority"]
[null,null,null,20232,null,"53_29/07/2021 1:54:15 PM","2021-07-09T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Ramp on main deck to be derusted.","Deck - Pipe / Fittings","General Appearance","External Factors","11.3","Medium","","","Main deck Ramps derusted and painted.","2021-08-09T23:59:35","","Completed","2021-07-16T23:59:35","No","No","No","Internal"]
[null,null,null,20233,null,"53_29/07/2021 1:57:05 PM","2021-07-09T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Chain blocks to be oiled.","Miscellaneous","Safety / LSA / FFA","Equipment Related","8.5","Very High","","","Oiling of Chain blocks carried out.","2021-08-09T23:59:35","","Completed","2021-07-09T23:59:35","No","No","No","Internal"]
[null,null,null,20234,null,"53_29/07/2021 1:59:59 PM","2021-07-09T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Canvas cover for Fwd Horn & Port search light to be renewed.","Deck - Machinery","General Appearance","Equipment Related","12.12","High","","","Canvas Cover renewed for Fwd Horn & port search light.","2021-08-09T23:59:35","","Completed","2021-07-15T23:59:35","No","No","No","Internal"]
[null,null,null,20235,null,"53_29/07/2021 2:06:15 PM","2021-07-09T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Spot maintenance of Hydraulic lines of remote mooring winch operating M5 to be carried out on main deck.","Deck - Mooring Machinery","Mooring","Equipment Related","9.14","Medium","","","Spot maintenance of Hydraulic lines of remote mooring winch operating M5 carried out on main deck.","2021-08-09T23:59:35","","Completed","2021-07-19T23:59:35","No","No","No","Internal"]
[null,null,null,20236,null,"53_29/07/2021 2:09:06 PM","2021-07-09T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","There are big wooden boxes which are not labelled as to what spare are inside.","Miscellaneous","General Appearance","External Factors","10.29","Medium","","","Big wooden boxes labelled as to what spare are inside.","2021-08-09T23:59:35","","Completed","2021-07-22T23:59:35","No","No","No","Internal"]
[null,null,null,23838,null,"53_31/01/2022 8:40:49 PM","2021-07-09T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Cover for Waste oil tank to renew","E/R - Pipes/ valves & fittings","Structural Condn. / WT integrity ","Equipment Related","6.9","Low","","","Vent cover removed, fabricated and renewed.","2021-08-24T23:59:35","","Completed","2021-08-23T23:59:35","No","No","No","Internal"]
[null,null,null,23839,null,"53_31/01/2022 8:45:00 PM","2021-07-09T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Main engine Bearing wear monitoring system frequent alarm due to faulty sensors.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Sensors received and renewed.","2021-10-08T23:59:35","","Completed","2021-10-01T23:59:35","No","No","No","Internal"]
[null,null,null,23840,null,"53_31/01/2022 8:49:07 PM","2021-07-09T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ME HPS System electric start up pump is unable to change over from MOP to select as master.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Advise received from makers. Sytem configured as per advise. System found changing oversatisfactorily","2021-10-08T23:59:35","","Completed","2021-07-29T23:59:35","No","No","No","Internal"]
[null,null,null,23841,null,"53_31/01/2022 8:52:06 PM","2021-07-09T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","To fabricate/ repair two air intake filter flaps for AC air handling unit.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","New intake filter flap fabricated and fitted.","2021-08-08T23:59:35","","Completed","2021-07-29T23:59:35","No","No","No","Internal"]
[null,null,null,20518,null,"53_20/08/2021 2:38:33 PM","2021-07-26T23:59:35","Defect","Ship Staff","Engineering Audit","Falty alarm from Fish room gas leak sensor.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","Sensor renewed. Found no alarm.","2021-11-24T23:59:35","DPUM210122","Completed","2021-08-03T23:59:35","No","No","No","Internal","spares approved; followup with procure for connections at Singapore this call"]
[null,null,null,20519,null,"53_20/08/2021 2:41:28 PM","2021-07-26T23:59:35","Defect","Ship Staff","Engineering Audit","No2 ECR AC trips frequently due to faulty controller.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Controller to be renewed. SPARE RECEIVED AND REPLACED.","2021-11-24T23:59:35","DPUM210121.","Completed","2021-09-24T23:59:35","No","No","No","Internal","Spares ready for connection this call Singapore; follow up with Procure team"]
[null,null,null,20709,null,"53_26/08/2021 12:21:00 PM","2021-08-10T23:59:35","Defect","Ship Staff","Engineering Audit","Crew mess room exhaust fan is defective and running noicy.","Accommodation,Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","Motor with fan to be renewed. Fan renewed","2021-11-24T23:59:35","DPUM210128","Completed","2021-09-30T23:59:35","No","No","No","Internal","ok, spares to be arranged as per ship request."]
[null,null,null,20711,null,"53_26/08/2021 1:35:04 PM","2021-08-17T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Pumproom Gas detection Fault Alarm","Miscellaneous","Safety / LSA / FFA","Equipment Related","5.17","Very High","","","Pumproom gas detction fault alarm - Analyse pump flow failure alarm. Job completed.","2021-11-17T23:59:35","","Completed","2021-09-07T23:59:35","No","No","No","Internal","follow up with Auto dept and F3 if any assistance required"]
[null,null,null,20710,null,"53_26/08/2021 12:27:57 PM","2021-08-18T23:59:35","Defect","Ship Staff","Engineering Audit","No 2 Deck seal pump motor ND end bearing housing has been worn out and motor found running noisy.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","New motor received and fitted.Found working satisfactorily.","2021-10-24T23:59:35","DPUM210142","Completed","2021-10-02T23:59:35","No","No","No","Internal","noted and new motor confirmed for supply"]
[null,null,null,20712,null,"53_02/09/2021 11:01:55 AM","2021-08-25T23:59:35","Defect","Ship Staff","Engineering Audit","No1 Composit boiler HFO pump mechanical seal leaking.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Overhaued the pump.","2021-11-24T23:59:35","","Completed","2021-08-29T23:59:35","No","No","No","Internal"]
[null,null,null,21102,null,"53_6/9/2021 1:23:35 PM","2021-08-29T23:59:35","Defect","Ship Staff","Engineering Audit","Salinometer for the Cascade tank outlet water is defective.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Reniew the PCB/ salinometer. NEW SALINOMETER RECEIVED AND FITTED. CALIBRATED AND WORKING GOOD.","2021-12-24T23:59:35","DPUM210168","Completed","2021-09-24T23:59:35","No","No","No","Internal","spares confirmed ; to be connected soon"]
[null,null,null,21101,null,"53_12/09/2021 1:12:48 PM","2021-09-05T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Ballast Line hole on No. 2 WBP pipeline between BA038 & BWTS Filter.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.8","Medium","","","Ballast Pipeline removed from location and take to engineroom workshop for welding.","2021-09-23T23:59:35","","Completed","2021-09-09T23:59:35","No","No","No","Internal","job completed to be closed out"]
[null,null,null,21103,null,"53_16/09/2021 8:25:43 AM","2021-09-08T23:59:35","Observation","Ship Staff","Ship Staff Insp.","STBD Side Draft Gauge showing eratic reading.","Miscellaneous","Cargo / Ballast Systems","Equipment Related","","","","","Presently it is showing maximum draft of 24meter. During investigation, found the level gradually increasing to maximum draft. So, the safety chamber was opened up for inspection.  Found to be in good order. Later, pneumatic modulator was overhauled. We suspect, Composition type pneumatic modulator is faulty. Modulator renewed and found working satisfactorily","2021-12-08T23:59:35","DPUM210176","Completed","2022-01-08T23:59:35","No","No","No","Internal","Spares processed for supply from makers"]
[null,null,null,21341,null,"53_02/10/2021 1:38:37 PM","2021-09-22T23:59:35","Defect","Ship Staff","Engineering Audit","System failure alarm on AMS. FMS no data connnection.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Trouble shooting in progress with the maker.System found found working satisfactorily.","2021-10-24T23:59:35","","Completed","2021-10-24T23:59:35","No","No","No","Internal","troubleshooting in progress with IT and makers.\nkindly follow up"]
[null,null,null,21514,null,"53_13/10/2021 12:46:29 PM","2021-10-05T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Pump room fixed Gas detection alarm.","Miscellaneous","Safety / LSA / FFA","Equipment Related","5.21","Medium","","","ALL LINES IN PUMP ROOM BLOWN THROUGH , SYSTEM WORKING , KEPT UNDER OBSERVATION.","2022-01-05T23:59:35","","Completed","2021-11-19T23:59:35","No","No","No","Internal","kindly follow up in separate mail if tech assistance required. complete and close out as planned."]
[null,null,null,23317,null,"53_02/11/2021 14:31:59","2021-10-08T23:59:35","Defect","Ship Staff","Ship Staff Insp.","FOUND DECK SEAL SW OUTLET VALVE & FLOW ALARM CONNECTION PIPE LEAKING","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","11.4","Very High","","","VALVE GLAND PACKING RENEWED. CONNECTION LEAKAGE RECTIFIED","2021-10-13T23:59:35","","Completed","2021-10-13T23:59:35","No","No","No","Internal"]
[null,null,null,23318,null,"53_02/11/2021 14:37:12","2021-10-08T23:59:35","Defect,Observation","Ship Staff","Ship Staff Insp.","PORT WINDLASS HYDRAULIC HOSE-POSITION -19,PART NO.002603.00550, DWG-1095789.002/001, FOUND LEAKING.","Deck - Mooring Machinery","Mooring","Equipment Related","11.14","Medium","","","HOSE RENEWED.","2021-10-08T23:59:35","","Completed","2021-10-08T23:59:35","No","No","No","Internal"]
[null,null,null,23319,null,"53_02/11/2021 14:40:41","2021-10-08T23:59:35","Defect","Ship Staff","Ship Staff Insp.","ENGINE ROOM BOTTOM FLOOR HEATING STEAM LINE (4K) LEAKING FROM FLANGE","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","11.4","Very High","","","4K STEAM LINE ISOLATED,GASKET RENEWED.","2021-10-09T23:59:35","","Completed","2021-10-08T23:59:35","No","No","No","Internal"]
[null,null,null,23320,null,"53_02/11/2021 14:44:56","2021-10-08T23:59:35","Defect","Ship Staff","Ship Staff Insp.","FWG EJECTOR PUMP MECHANICAL SEAL LEAKING","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","11.4","Very High","","","FWG EJECTOR PUMP- OPENED UP / INSPECT ALL PARTS.FOUND MECHANICAL SEAL WORN. ALSO FOUND SHAFT SLEEVE LOOSE ON SHAFT AND TURNING FREELY. IMPELLER FOUND INTACT. ALL PARTS CLEANED IND INSPECTED. \n\nPUMP ASSEMBLED WITH NEW MECHANICAL SEAL, SLEEVE AND SHAFT AND CORRECTLY ALIGNED WITH MOTOR. PUMP IS TESTED AND FOUND ALL PARAMETERS NORMAL AND NO VIBRATION / NO LEAKS.\n\n","2021-11-08T23:59:35","","Completed","2021-10-15T23:59:35","No","No","No","Internal"]
[null,null,null,22884,null,"53_15/10/2021 6:26:50 PM","2021-10-08T23:59:35","Defect","Ship Staff","Ship Staff Insp.","FOUND DECK SEAL SW OUTLET VALVE GLAND & FLOW ALARM CONNECTION PIPE LEAKING.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","11.4","Very High","","","VALVE GLAND PACKING IS RENEWED AND PIPE CONNECTIONLEAK RECTIFIED.","2021-11-08T23:59:35","","Completed","2021-10-13T23:59:35","No","No","No","Internal"]
[null,null,null,22885,null,"53_25/10/2021 13:23:43","2021-10-08T23:59:35","Defect,Observation","Ship Staff","Ship Staff Insp.","PORT WINDLASS FLEXIBLE HYDRAULIC HOSE-POSITION -19, PART NO.002603.00550, DWG-1095789.002/001","Deck - Mooring Machinery","Mooring","Behaviour Based","11.14","Medium","","","HYDRAULIC- FLEXIBLE HOSE IS RENEWED WITH SPARE HOSE.","2021-11-09T23:59:35","","Completed","2021-10-08T23:59:35","No","No","No","Internal"]
[null,null,null,22886,null,"53_25/10/2021 13:33:23","2021-10-08T23:59:35","Defect,Observation","Ship Staff","Ship Staff Insp.","ENGINE ROOM BOTTOM FLOOR HEATING STEAM LINE (4k) FLANGE LEAKAGE.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Behaviour Based","11.4","Very High","","","4k STEAM LINE ISOLATED & PIPE FLANGE GASKET IS  RENEWED. WITH METAFLEX GASKET.","2021-10-09T23:59:35","","Completed","2021-10-08T23:59:35","No","No","No","Internal"]
[null,null,null,23311,null,"53_01/11/2021 5:36:59 PM","2021-10-09T23:59:35","Defect","Ship Staff","Ship Staff Insp.","WBT fixed gas detection system found void space flow failure fault","Miscellaneous","Cargo / Ballast Systems","Equipment Related","5.23","Very High","","","Line blown through and cleared.Found working satisfactorily.","2021-11-23T23:59:35","","Completed","2021-11-11T23:59:35","No","No","No","Internal","procedure provided and issue resolved"]
[null,null,null,22883,null,"53_25/10/2021 6:28:12 PM","2021-10-09T23:59:35","Defect","Ship Staff","Ship Staff Insp.","1 No portable multigas detector GX2009 battery failure. Not charging and inoperational.","Miscellaneous","Safety / LSA / FFA","Equipment Related","5.23","Very High","","","Battery renewed","2021-11-23T23:59:35","","Completed","2022-01-02T23:59:35","No","No","No","Internal","spares supplied at Singapore 09th Jan"]
[null,null,null,22887,null,"53_25/10/2021 13:01:49","2021-10-09T23:59:35","Defect,Observation","Ship Staff","Ship Staff Insp.","FWG EJECTOR PUMP FOUND LEAKAGE FROM MECHANICAL SEAL.","E/R - Pumps","Eng. / Strg. Comp.","Behaviour Based","11.4","Very High","","","FWG EJECTOR PUMP- OPENED UP / INSPECT ALL PARTS.FOUND MECHANICAL SEAL WORN. ALSO FOUND SHAFT SLEEVE LOOSE ON SHAFT AND TURNING FREELY. IMPELLER FOUND INTACT. ALL PARTS CLEANED IND INSPECTED. \n\nPUMP ASSEMBLED WITH NEW MECHANICAL SEAL, SLEEVE AND SHAFT AND CORRECTLY ALIGNED WITH MOTOR. PUMP IS TESTED AND FOUND ALL PARAMETERS NORMAL AND NO VIBRATION / NO LEAKS.\n\n","2021-11-08T23:59:35","","Completed","2021-10-15T23:59:35","No","No","No","Internal"]
[null,null,null,22888,null,"53_25/10/2021 6:30:48 PM","2021-10-09T23:59:35","Defect","Ship Staff","Ship Staff Insp.","WBT Fixed gas detection system fwd void space flow failure fault","Miscellaneous","Safety / LSA / FFA","Equipment Related","5.23","Very High","","","Line blown through and cleared. Found working satisfactorily","2021-11-23T23:59:35","","Completed","2021-11-11T23:59:35","No","No","No","Internal"]
[null,null,null,23321,null,"53_02/11/2021 13:33:04","2021-10-16T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Aft hydraulic cooler sea water inlet and oulet lines have slight leakage from pipe seam","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","5.42","Medium","","","Pipes fabricated and renewed.","2021-10-24T23:59:35","","Completed","2021-10-24T23:59:35","No","No","No","Internal"]
[null,null,null,22889,null,"53_25/10/2021 13:39:35","2021-10-16T23:59:35","Defect,Observation","Ship Staff","Ship Staff Insp.","AFT HYDRAULIC MACHINERY COOLER SEA WATER IN/OUT LINES SW LEAKAGES.","Deck - Mooring Machinery,Deck - Pipe / Fittings","Eng. / Strg. Comp.","Behaviour Based","11.4","Very High","","","Pipe section fabricated and renewed.","2021-11-15T23:59:35","","Completed","2021-10-24T23:59:35","No","No","No","Internal"]
[null,null,null,23312,null,"53_03/01/2022 1:14:22 PM","2021-10-18T23:59:35","Defect","Ship Staff","Ship Staff Insp.","BWTS NO 1 FILTER INLET PRESSURE TRANSMITTER FAULTY.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.5","Very High","","","PRESSURE TRANSMITTER RECEIVED AND RENEWED","2022-01-23T23:59:35","DPUM-210186 ","Completed","2022-03-23T23:59:35","No","No","No","Internal","complete on priority... spares received onboard"]
[null,null,null,23310,null,"53_03/11/2021 4:29:18 PM","2021-10-27T23:59:35","Defect","Ship Staff","Nav Audit / Verification","Inclinometer dimmer not working.Pottentiometer found not working.","Navigation - Others","Navigation","Equipment Related","4.3","Medium","","","Potentiometer renewed and tried out. Found dimmer operating satisfactory.","2022-01-24T23:59:35","DPUM210193.","Completed","2022-03-22T23:59:35","No","No","No","Internal","complete on receipt of spares and close out"]
[null,null,null,23313,null,"53_02/11/2021 14:26:40","2021-10-30T23:59:35","Defect","Ship Staff","Ship Staff Insp.","SLIGHT LEAK FROM # 1 STEERING JENNY PUMP NDE COVER","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","","","","","End cover screws slackened and retightened evenly.Leak has stopped.Under observation.","2022-01-18T23:59:35","DPUM210192","Completed","2022-02-20T23:59:35","No","No","No","Internal","please follow up with purchase for spares readiness and plan close out at the earliest"]
[null,null,null,23322,null,"53_03/01/2022 10:32:02","2021-11-10T23:59:35","Defect","Ship Staff","Ship Staff Insp.","SHAFT EARTHING DEVICE SHOWING ERRATIC VALUE.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","11.1","High","","","CARBON BRUSHES RENEWED.","2021-12-24T23:59:35","DPUM210199","Completed","2021-11-11T23:59:35","No","No","No","Internal"]
[null,null,null,23346,null,"53_05/01/2022 5:14:22 PM","2021-11-10T23:59:35","Defect","Ship Staff","Ship Staff Insp.","SHAFT EARTHING DEVICE SHOWING ERRATIC VALUE","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","11.1","High","","","CARBON BRUSHES RENEWED","2021-12-24T23:59:35","DPUM210199","Completed","2021-11-11T23:59:35","No","No","No","Internal"]
[null,null,null,22890,null,"53_30/11/2021 2:13:18 PM","2021-11-13T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Fresh water generator feed water line leaking from union","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.1","Medium","","","Pipe removed. Found corroded at union section. Pipe renewed and fitted.","2021-11-15T23:59:35","","Completed","2021-11-14T23:59:35","No","No","No","Internal"]
[null,null,null,23323,null,"53_03/01/2022 10:36:32","2021-12-13T23:59:35","Defect","Ship Staff","Ship Staff Insp.","M/E FO #1 CIRCULATING PUMP RUNNING WITH SLIGHT NOISE.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","","","","","PUMP DISMANTLED.BEARING FOUND DAMAGED AND SHAFT WORN.BEARINGS AND SHAFT RENEWED.PUMP ASSEMBLED AND TRIED OUT SATISFACTORILY ","2021-12-18T23:59:35","","Completed","2021-12-15T23:59:35","No","No","No","Internal"]
[null,null,null,23347,null,"53_05/01/2022 5:18:34 PM","2021-12-13T23:59:35","Defect","Ship Staff","Ship Staff Insp.","M/E FO CIRCULATING PIMO RUNNING WITH SLIGHT NOISE","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","11.1","High","","","PUMP DISMANTLED.BEARING FOUND DAMAGED AND SHAFT WORN.BEARINGS AND SHAFT RENEWED.PUMP ASSEMBLED AND TRIED OUTSATISFACTORILY","2021-12-18T23:59:35","","Completed","2021-12-15T23:59:35","No","No","No","Internal"]
[null,null,null,23836,null,"53_04/02/2022 1:21:56 PM","2022-01-02T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","The electric motor overhauling plan to submit along with targets to cover all motors within 6 months.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Motor list is in use with motor overhaul schedule and being followed and updated.","2022-03-01T23:59:35","","Completed","2022-02-04T23:59:35","No","No","No","Internal","list to be forwarded on weekly basis with other weekly jobs"]
[null,null,null,23837,null,"53_04/02/2022 5:08:07 PM","2022-01-02T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Both manifolds areas ( main deck and tray area) to upgrade cosmetically as some rust sign are seen on manifold area.","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.4","Very High","","","Both manifolds areas Chipped and painted ( main deck and tray area) ","2022-04-01T23:59:35","","Completed","2022-03-08T23:59:35","No","No","No","Internal","complete as planned and close out"]
[null,null,null,23842,null,"53_04/02/2022 1:18:14 PM","2022-01-02T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ME performance and DG performance to be strictly recorded at 85% every month and compare the same with sea trial reports. All data from COCOS to be analyzed and sent monthly and attach in PAL.","E/R - Aux. Engine,E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Performance recorded and analyzed.Report attached in PAL.","2022-02-21T23:59:35","","Completed","2022-01-24T23:59:35","No","No","No","Internal"]
[null,null,null,23843,null,"53_04/02/2022 1:24:14 PM","2022-01-02T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Steering gear room rudder grease pump operation to check and confirm that all lines are clear and report the daily or weekly  grease consumption. ","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Grease consumption being recorded daily","2022-02-01T23:59:35","","Completed","2022-01-27T23:59:35","No","No","No","Internal"]
[null,null,null,24127,null,"53_04/02/2022 12:48:49 PM","2022-01-02T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","There is minor oil leak noticed on ME Exhaust valve actuators on units 1,2 and 3. ","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Leak identified to lower plug.Plugs removed.Threads and seal ring cleaned,inspected and torque tightened after putting thread lock liquid.No leaks observed.","2022-03-01T23:59:35","","Completed","2022-02-24T23:59:35","No","No","No","Internal"]
[null,null,null,24128,null,"53_13/02/2022 12:36:30 PM","2022-01-02T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Both manifold areas(main deck and tray areas) to upgrade cosmetically as some rust signs are seen on manifold area","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.4","Very High","","","Both manifold areas(main deck and tray areas), chipped and Painted","2022-04-01T23:59:35","","Completed","2022-03-08T23:59:35","No","No","No","Internal"]
[null,null,null,24129,null,"53_13/02/2022 12:40:02 PM","2022-01-02T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","There is minor leak noticed on M/E exhaust actuator 1,2 and 3","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Leak identified to lower plug.Plugs removed.Threads and seal ring cleaned,inspected and torque tightened after putting thread lock liquid.No leaks observed.","2022-04-01T23:59:35","","Completed","2022-02-24T23:59:35","No","No","No","Internal"]
[null,null,null,24130,null,"53_13/02/2022 12:44:03 PM","2022-01-02T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Hydraulic pipelines-VRCS and mooring lines U-Clamp and pipe support needs maintenance on few locations particularly expansion joints to be covered properly with good surface preperation and stripe coat of epoxy.","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.4","Very High","","","Job completed","2022-04-01T23:59:35","","Completed","2022-03-28T23:59:35","No","No","No","Internal"]
[null,null,null,24134,null,"53_04/02/2022 12:39:38 PM","2022-01-02T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ME performance and DG performance to be strictly recorded at 85% every month and compare the same with sea trial reports. All data from COCOS to be analyzed and sent monthly and attach in PAL.","E/R - Aux. Engine,E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Performance recorded and compared with sea trial data.Uploaded in PAL","2022-02-21T23:59:35","","Completed","2022-01-24T23:59:35","No","No","No","Internal"]
[null,null,null,24135,null,"53_04/02/2022 12:43:07 PM","2022-01-02T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","The electric motor overhauling plan to submit along with targets to cover all motors within 6 months.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Motor overhauling schedule tabulated in Excel sheet being followed and updated.Motors due in next 6 months identified and spares checked","2022-02-01T23:59:35","","Completed","2022-02-04T23:59:35","No","No","No","Internal"]
[null,null,null,24136,null,"53_04/02/2022 12:46:07 PM","2022-01-02T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Sewage treatment plant – EVAC pp daily running hours to be recorded by duty engr.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Evac pump does not have run hour counter.Pump operation being monitored closely.Vaccuume system being checked regularly for leaks.","2022-02-01T23:59:35","","Completed","2022-01-25T23:59:35","No","No","No","Internal"]
[null,null,null,24137,null,"53_04/02/2022 12:52:22 PM","2022-01-02T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Incinerator to be operated atleast every 15 days in sludge for full day and record same in Oil record book.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Incinerator being run every week on sludge during manned period.","2022-03-01T23:59:35","","Completed","2022-02-06T23:59:35","No","No","No","Internal"]
[null,null,null,24138,null,"53_04/02/2022 12:55:23 PM","2022-01-02T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Steering gear room rudder grease pump operation to check and confirm that all lines are clear and report the daily or weekly  grease consumption.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Daily consumption is being recorded.","2022-02-01T23:59:35","","Completed","2022-01-27T23:59:35","No","No","No","Internal"]
[null,null,null,24139,null,"53_13/02/2022 12:46:49 PM","2022-01-02T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Port side lifeboat davit drum handle securing to renew","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.28","Very High","","","Securing arrangement renewed.","2022-03-02T23:59:35","","Completed","2022-01-28T23:59:35","No","No","No","Internal"]
[null,null,null,24140,null,"53_13/02/2022 12:53:42 PM","2022-01-02T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","All cargo dome cover wing nuts and closing covers to be greased and made free.","Cargo Mach.,Deck - Machinery,Deck - Pipe / Fittings","Structural Condn. / WT integrity ","Equipment Related","8.21","High","","","Cargo domes and wing nuts eased and greased","2022-02-02T23:59:35","","Completed","2022-01-13T23:59:35","No","No","No","Internal"]
[null,null,null,24141,null,"53_13/02/2022 12:49:33 PM","2022-01-02T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Valve handles for Slop tank steam heating coils is broken.Same to renew.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","11.4","Very High","","","Valve handles renewed.","2022-03-02T23:59:35","","Completed","2022-01-26T23:59:35","No","No","No","Internal"]
[null,null,null,24131,null,"53_13/02/2022 12:59:19 PM","2022-02-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","BWTS Rectifier # 1 SCR and current limiting fuse busted","Deck - Machinery","Cargo / Ballast Systems","Equipment Related","6.21","High","","","SCR and fuse busted due to water leak from cooler NR valve.all Spares received except SCR.","2022-05-08T23:59:35","DPUM220034","Completed","2022-05-08T23:59:35","No","No","No","Internal","Fuses were connected to ship; can the job be completed. other spares ready for connection at next available opportunity."]
[null,null,null,24132,null,"53_02/03/2022 1:09:09 PM","2022-02-16T23:59:35","Defect","Ship Staff","Ship Staff Insp.","AFT PEAK TANK LEVEL GAUGE SHOWING ERRATIC VALUES AND DISPLAYING SENSOR FAIL ALARM","Hull & Tanks","Cargo / Ballast Systems","Equipment Related","8.12","Medium","","","MODULATOR CHECKED AND FOUND OUTPUT SIGNAL MORE THAN 31 MA.DIAPHRAGM FOUND GOOD.SENSOR FAULTY.RO RAISED.","2022-05-18T23:59:35","DPUM220041","Completed","2022-05-18T23:59:35","No","No","No","Internal","spares will be connected as per RO. once the quotes are received"]
[null,null,null,25134,null,"53_21/04/2022 18:54:58","2022-03-15T23:59:35","Defect,Observation","Ship Staff","Ship Staff Insp.","BWTS,A3 module are out of operation due to burnt condition of cell guide plates.","Cargo Mach.,Elect. Mach. & Equip.","Cargo / Ballast Systems","Equipment Related,External Factors,Inappropriate Procedure","6.21","High","","","Need to be renewed complete Electolyzer modules A3.\nAwaiting spare. 2nd Jan 2023 DDRL it is due , 31st Jan missing from due AND completed. This job has been re entered regarding damaged bipolar plates of APT BWTS system.-Please advise if this can be closed in current date. CLOSED AS SAME RAISED AGAIN FOR 2023","2022-09-24T23:59:35","DPUM220200","Completed","2022-12-30T23:59:35","No","No","Yes","Internal","The RO raised was in 2022, the vessel docked in Dec 2022. \n\nwhat is the present status of this issue?"]
[null,null,null,25135,null,"53_22/04/2022 14:17:23","2022-03-16T23:59:35","Defect","Ship Staff","Ship Staff Insp.","AUX BOILER COMMON ATMOSING PRESSURE STEAM LINE PR. SWITCH MALFUNCTIONING","Cargo Mach.,E/R - Boiler","Eng. / Strg. Comp.","Equipment Related,External Factors,Human Error,Inappropriate Procedure","10.32","Very High","","","AT PRESENT SWITCH HAS BEEN  RENEWED.","2022-06-23T23:59:35","DPUM220062","Completed",null,"No","No","No","Internal"]
[null,null,null,24700,null,"53_02/04/2022 11:58:58 AM","2022-03-18T23:59:35","Defect","Ship Staff","Ship Staff Insp.","AUX BOILER FO SUPPLY PUMP LEAKING FROM SEAL","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","","","","","PUMP DISMANTLED. SEALS AND BEARING RENEWED.PUMP TRIED OUT AND FOUND NO LEAKS.","2022-03-27T23:59:35","","Completed","2022-03-24T23:59:35","No","No","No","Internal"]
[null,null,null,25136,null,"53_21/04/2022 11:27:16 PM","2022-04-04T23:59:35","Observation","Ship Staff","Ship Staff Insp.","In Fixed Gas Detection system, P/Room H2S detector are malfunctioning for reading.\n\n\n\n","Cargo Mach.,Elect. Mach. & Equip.","Cargo / Ballast Systems","Equipment Related,External Factors,Inappropriate Procedure","8.46","Very High","","","Valid bottle of test gas are applied from P/Room as well as from local but not indicating any readings,zero and Spantried out as per advised POT is adjusted for span but in actual readings are not available,troubleshooting is in progress.","2022-07-02T23:59:35","DPUM220077","Completed","2022-06-24T23:59:35","No","No","No","Internal"]
[null,null,null,25137,null,"53_17/04/2022 15:46:28","2022-04-07T23:59:35","Defect,Observation","Ship Staff","Ship Staff Insp.","#2 Composite Boiler FO Pumps leaking from shaft seal.","E/R - Boiler,E/R - Pumps","Eng. / Strg. Comp.","Equipment Related,External Factors,Human Error,Inappropriate Procedure","10.32","Very High","","","Pump Has been overhauled and found in good order","2022-07-07T23:59:35","","Completed",null,"No","No","No","Internal"]
[null,null,null,25561,81209,"53_Sat Apr 30 2022 08:45:50 GMT+0800","2022-04-15T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Fresh Water Minerlizer inlet 3-way valve are not holding for water.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Inappropriate Procedure,Equipment Related,External Factors","10.32","Very High","","","Valve to be Renewed.","2022-07-15T23:59:35","DPUM220092","Completed","2022-05-18T23:59:35","No","No","No","Internal"]
[null,null,null,25555,26208,"53_Sat Apr 30 2022 08:43:27 GMT+0800","2022-04-19T23:59:35","Defect,Observation","Ship Staff","Ship Staff Insp.","Incinerator sluice door solenoid air block found in powder form and air is leaking through the body.Temporarily air has been shut by adding blank.","E/R - Aux. Mach.,Elect. Mach. & Equip.","MARPOL Related","Equipment Related,External Factors,Human Error,Inappropriate Procedure","10.32","Very High","","","Solenoid block to be renewed.","2022-07-19T23:59:35","DPUM220093","Completed","2022-06-16T23:59:35","No","No","No","Internal"]
[null,null,null,25554,59614,"53_Sat Apr 30 2022 08:39:26 GMT+0800","2022-04-22T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Personnel elevator floor identification buzzer not working inside the car.","E/R - Aux. Mach.,Elect. Mach. & Equip.","Eng. / Strg. Comp.","Inappropriate Procedure,Equipment Related,External Factors","10.32","Very High","","","Need to be Renewed.","2022-07-23T23:59:35","DPUM220094","Completed","2022-06-16T23:59:35","No","No","No","Internal"]
[null,null,null,26426,null,"53_Fri Aug 05 2022 01:00:50 GMT+0000","2022-05-08T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","4 NUMBERS OF COW MACHINE VALVES REPORTEDLY FOUND NOT HOLDING.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.34","High","","","SEAT RING RENEWED FOR COW MACHINE VALVES; NAMELY – 2C, 5C :  NO.2 DECK MOUNTED MACHINE V/V,  3S  FWD & 4P AFT DECK MOUNTED MACHINE V/V","2022-08-09T23:59:35","DPUM220129","Completed","2022-07-12T23:59:35","No","No","No","Internal"]
[null,null,null,25556,49547,"53_Fri May 20 2022 11:53:28 GMT+0800","2022-05-08T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","NO.1 & 2 CARGO EDUCTOR GAUGES REPORTED TO BE ERRATIC.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.8","Medium","","","CALIBRATION OF NO.1 & 2 CARGO EDUCTOR GAUGES CARRIED OUT,","2022-05-30T23:59:35","","Completed","2022-06-01T23:59:35","No","No","No","Internal"]
[null,null,null,25559,23119,"0_Mon May 16 2022 20:19:33 GMT+0800","2022-05-08T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","CLEAN BILGE TANK 15 PPM MEASURING UNIT NOT SET IN GMT TIME.","Elect. Mach. & Equip.","MARPOL Related","Human Error,Inappropriate Procedure","6.17","Very High","","","TIME TO BE SET GMT.","2022-05-08T23:59:35","","Completed","2022-05-08T23:59:35","No","No","No","Internal"]
[null,null,null,25560,80179,"0_Mon May 16 2022 20:23:58 GMT+0800","2022-05-08T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","IN CCR, CARGO CONSOLE PANEL NORMAL 220V & DC 24V POWER LAMPS FOUND IN FUSED CONDITION.","Cargo Mach.,Elect. Mach. & Equip.","Cargo / Ballast Systems","Equipment Related,Human Error,Inappropriate Procedure,External Factors","8.80","Medium","","","NEED TO BE RENEWED THE LAMPS","2022-06-08T23:59:35","","Completed","2022-05-09T23:59:35","No","No","No","Internal"]
[null,null,null,25562,55669,"53_Fri May 27 2022 10:46:48 GMT+0800","2022-05-08T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","FOUND SOME OF HANDHELD UHF TRANSRECIVERS (WALKIE TALKIES) TAPED WITH THE BATTERY","Miscellaneous","Communication","Behaviour Based","4.26","Low","","","SAME RECTIFIED & ALL IN USE WALKIE TALKIES STENCILED.","2022-06-07T23:59:35","","Completed","2022-05-15T23:59:35","No","No","No","Internal"]
[null,null,null,25563,23646,"0_Fri May 27 2022 10:51:00 GMT+0800","2022-05-08T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","P & S ACCOMODATION LADDER SHEAVES REQUIRE GREASING.","Deck - Machinery","General Appearance","External Factors","11.4","Very High","","","GREASING OF P & S ACCOMODATION LADDER SHEAVES CARRIED OUT.","2022-06-07T23:59:35","","Completed","2022-05-13T23:59:35","No","No","No","Internal"]
[null,null,null,25564,73892,"0_Fri May 27 2022 10:57:53 GMT+0800","2022-05-08T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","LASHING WIRE TO BE RENEWED FOR PORT SIDE PILOT LADDER STORAGE DRUM","Deck - Machinery","General Appearance","Equipment Related","11.4","Very High","","","LASHING WIRE RENEWED FOR PORT SIDE PILOT LADDER STORAGE DRUM","2022-06-07T23:59:35","","Completed","2022-05-19T23:59:35","No","No","No","Internal"]
[null,null,null,25565,36128,"53_Fri May 27 2022 11:00:19 GMT+0800","2022-05-08T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","P & S FWD CHAIN STOPPER RUSTING","Deck - Mooring Machinery","Mooring","External Factors","11.4","Very High","","","DERUSTING & PAINTING OF P & S FWD CHAIN STOPPER CARRIED OUT.","2022-06-07T23:59:35","","Completed","2022-05-16T23:59:35","No","No","No","Internal"]
[null,null,null,25566,81152,"0_Fri May 27 2022 11:08:17 GMT+0800","2022-05-08T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","IG DECK WATER SEAL FILLING LINE RUSTING","Deck - Pipe / Fittings","General Appearance","External Factors","11.4","Very High","","","DERUSTING & PAINTING OF IG DECK WATER SEAL FILLING LINE CARRIED OUT.","2022-06-07T23:59:35","","Completed","2022-05-14T23:59:35","No","No","No","Internal"]
[null,null,null,25567,41879,"0_Fri May 27 2022 11:09:43 GMT+0800","2022-05-08T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","FIRE LINE IN FWD BOSUN STORE RUSTING","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.4","Very High","","","DERUSTING & PAINTING OF FIRE LINE IN FWD BOSUN STORE CARRIED OUT.","2022-06-07T23:59:35","","Completed","2022-05-16T23:59:35","No","No","No","Internal"]
[null,null,null,25568,96526,"0_Mon May 16 2022 20:22:02 GMT+0800","2022-05-08T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","BOTH AUX BLR FO BURN PUMP UNITS MECHANICAL SEAL SEALING OIL POT SIGHT GLASS NOT VISIBLE AND OIL LEVEL IS NOT ENOUGH","","Eng. / Strg. Comp.","Human Error,Inappropriate Procedure,Equipment Related,Knowledge Based","10.32","Very High","","","NEED TO BE CLEANED THE POT/SIGHT GLASS AND FILL THE SUFFICIENT LEVEL OF OIL.","2022-06-08T23:59:35","","Completed","2022-05-10T23:59:35","No","No","No","Internal"]
[null,null,null,25569,90570,"0_Fri May 27 2022 10:52:47 GMT+0800","2022-05-08T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","EMULSIFIED GEAR OIL OBSERVED IN MW1, MW2 & MW3 WINCHES","Deck - Mooring Machinery","Mooring","External Factors","9.14","Medium","","","GEAR OIL RENEWED FOR MW1, MW2 & MW3  WINCHES.","2022-06-07T23:59:35","","Completed","2022-05-21T23:59:35","No","No","No","Internal"]
[null,null,null,25570,98835,"53_Mon May 16 2022 20:17:27 GMT+0800","2022-05-08T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","IN PURIFIER ROOM, SOME OF THE PIPE PORTION INSULATION MISSING OR ALREADY IN TORN CONDITION","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Human Error,External Factors,Equipment Related,Inappropriate Procedure","10.32","Very High","","","NEED TO BE INSTALLED FRESH INSULATION AND REPAIR","2022-06-08T23:59:35","","Completed","2022-05-21T23:59:35","No","No","No","Internal"]
[null,null,null,25973,79299,"53_Sat Jun 04 2022 02:24:00 GMT+0800","2022-05-09T23:59:35","Observation,Defect","Ship Staff","Ship Staff Insp.","In BWTS room,Main Ballast system FIT-1131 Flow meter PCB Malfunctioning","Cargo Mach.","Cargo / Ballast Systems","External Factors,Equipment Related,Industry Issue","6.21","High","","","Flow meter malfunctioning sometimes. PCB need renewal for permanent repair.\nSPARE RECEIVED AND WILL BE INSTALL DURING BWTS UPGRADITION. Understand this FM is for aft peak system. Can test only when Aft peak system is operational. ( From DDRL sheet sent on 16/05/23). target date revised  from 25/09/22. Raised again in 2023- being closed for 2022.","2023-12-30T23:59:35","DPUM220153","Completed","2022-12-29T23:59:35","No","No","Yes","Internal","Noted that spares was received as per DPUM220153. \nWhat is the present status of this Main Ballast system FIT-1131 Flow meter PCB Malfunctioning."]
[null,null,null,30640,57198,"0_Mon Mar 13 2023 13:25:18 GMT+0800","2022-05-12T23:59:35","Critical Equipment,Defect","Owner / Marine / Tech. Suptd.","Nav Audit / Verification","DC lamp for magnetic compass was not bright to read the compass heading.","Navigation - Others","Navigation","Equipment Related","4.7","High","","","Degraded Bulb replaced with new spare bulb. Tested, DC lamp for magnetic compass is having  optimum brightness and is satisfactory.","2022-08-11T23:59:35","","Completed","2022-05-14T23:59:35","No","No","No","Internal"]
[null,null,null,25990,62192,"53_Thu Jun 09 2022 15:08:17 GMT+0800","2022-05-13T23:59:35","Observation","Ship Staff","Ship Staff Insp.","NAVTEX PRINTOUTS ARE NOT READABLE","Navigation - GMDSS & Communication","Navigation","Equipment Related","4.7","High","","","PRINTER PAPER REPLACE WITH NEW SUPPLIES, STILL ISSUE PERSISTS THE SAME. LATER INFORMED TO TECHNICAL DEPT. MR. KAMLESH SOLANKI ABOUT THE DEFECT. HE ADVISED THAT PRINTER HEAD NEEDS TO BE REPLACED WHICH WILL BE CARRIED OUT AT NEXT PORT OF CALL.","2022-08-13T23:59:35","DPUM220179 =  NAVTEX PRINTER @ SINGAPORE","Completed","2022-06-16T23:59:35","No","No","No","Internal"]
[null,null,null,26427,null,"53_Fri Aug 05 2022 01:04:08 GMT+0000","2022-05-19T23:59:35","Defect","Ship Staff","Ship Staff Insp.","ANEMOMETER HIGH LEVEL HORN MALFUNCTIONING FOR AUDIBLE ALARM","Navigation - Others","Navigation","External Factors","4.7","High","","","Need to be replaced the complete assembly. Spare received & fitted. OK now.",null,"DPUM220162","Completed","2022-07-21T23:59:35","No","No","No","Internal"]
[null,null,null,25553,74163,"53_Wed Jun 01 2022 06:50:05 GMT+0800","2022-05-20T23:59:35","Defect","Ship Staff","Ship Staff Insp.","During routine maintenance found Slop P IG branch valve(Butterfly valve) gear is broken.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.25","Very High","","","SLOP P IG Branch valve renewed & found in order now.","2022-08-19T23:59:35","DPUM220166","Completed","2022-06-20T23:59:35","No","No","No","Internal"]
[null,null,null,25571,39115,"0_Wed Jun 01 2022 06:53:27 GMT+0800","2022-05-21T23:59:35","Defect","Ship Staff","Ship Staff Insp.","During Routine maintenance found No.1 Fire/ Foam isolation valve was hard to open/ shut.","Deck - Pipe / Fittings","Safety / LSA / FFA","Equipment Related","5.38","High","","","Upon overhauling of valve found the valve spindle had slight bent, same been rectified & valve put back in use.","2022-06-27T23:59:35","","Completed","2022-05-21T23:59:35","No","No","No","Internal"]
[null,null,null,26811,null,"53_Fri Sep 16 2022 04:02:52 GMT+0000","2022-06-04T23:59:35","Defect","Ship Staff","Ship Staff Insp.","\"vessel observed steering gear#2 shaft seal are slightly leaking for oil. Approx. 0.5-0.7 liters oil collected in 24-hour time period.\n\"","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","pump overhauled by yard","2022-11-04T23:59:35","","Completed","2022-12-23T23:59:35","No","No","No","Internal","Wait for next opportunity when at open sea for renewal of lip seal."]
[null,null,null,30627,35740,"53_Mon Mar 13 2023 11:01:07 GMT+0800","2022-06-05T23:59:35","Observation","Ship Staff","Nav Audit / Verification","STEERING GEAR LIGHT WAS OBSERVED NOT RESPONDING TO DIMMER WHEN ADJUSTING THE BRIGHTNESS LEVEL.","Navigation - Others","Navigation","Equipment Related,Human Error","4.8","Medium","","","AFTER INVESTIGATION, FOUND LED BULB WAS FITTED ON STEERING LIGHT HOLDER. LED BULB WAS REPLACED WITH NORMAL FILAMENT BULB. STEERING LIGHT IS NOW WORKING SATISFACTORY AND BRIGHTNESS LEVELS CAN BE ADJUSTED AS REQUIRED FROM DIMMER INSIDE WHEELHOUSE.","2022-09-05T23:59:35","","Completed","2022-06-05T23:59:35","No","No","No","Internal"]
[null,null,null,30628,36002,"0_Mon Mar 13 2023 11:04:46 GMT+0800","2022-06-05T23:59:35","Observation","Ship Staff","Nav Audit / Verification","LSA/FFA WEEKLY CHECK ENTRIES WERE MISSING IN DECK LOG BOOK. ","Navigation - Others,LSA / FFA,Documentation","Safety / LSA / FFA","Human Error","5.27","Medium","","","SAME ENTRIES HAS BEEN COMPLETED.","2022-09-05T23:59:35","","Completed","2022-06-05T23:59:35","No","No","No","Internal"]
[null,null,null,30629,77488,"53_Mon Mar 13 2023 11:08:29 GMT+0800","2022-06-05T23:59:35","Observation","Ship Staff","Nav Audit / Verification","GMDSS LOG BOOK ENTRIES REQUIRE COMPARISON OF SHIP'S LT WITH UTC ONCE A DAY, TO BE RECORDED. SAME WAS NOT DONE","Navigation - GMDSS & Communication,Documentation","Navigation","Human Error,Knowledge Based","4.23","High","","","ENTRIES FOR RECORD OF COMPARISON OF LT & UTC HAS BEEN STARTED AS REQUIRED","2022-09-05T23:59:35","","Completed","2022-06-05T23:59:35","No","No","No","Internal"]
[null,null,null,30632,40272,"0_Mon Mar 13 2023 11:11:27 GMT+0800","2022-06-05T23:59:35","Observation","Ship Staff","Nav Audit / Verification","\"OFFICIAL LANGUAGE ONBOARD IS ENGLISH\" STICKER NOT PASTED ON ALL THE LOG BOOKS. ","Navigation - Others","Navigation","Inappropriate Procedure,Human Error","3.3","High","","","SAME HAS BEEN COMPLETED.\nWHENEVER ANY NEW LOGBOOK IS STARTED, STICKER TO BE PASTED OR HANDWRITTEN WORDINGS TO BE USED IN FRONT OF LOG BOOK, ","2022-09-05T23:59:35","","Completed","2022-06-05T23:59:35","No","No","No","Internal"]
[null,null,null,30634,21269,"0_Mon Mar 13 2023 11:14:53 GMT+0800","2022-06-05T23:59:35","Defect","Ship Staff","Nav Audit / Verification","NAVTEX PRINTOUTS ARE NOT READABLE. MAKER'S MANUAL RECOMMENDS TO REPLACE PRINTER AS NAVTEX PRINTER CAN PRINT ABOUT 90 THERMAL PAPER ROLLS ONLY IN ITS LIFESPAN.","Navigation - GMDSS & Communication","Navigation","Equipment Related","4.7","High","","","NEW NAVTEX PRINTER RECEIVED VIDE RO DPUM22017 AT SINGAPORE. SAME REPLACED. NAVTEX PRINTOUTS ARE READABLE AND SATISFACTORY. ","2022-09-05T23:59:35","DPUM22017","Completed","2023-06-20T23:59:35","No","No","No","Internal"]
[null,null,null,30635,35746,"0_Mon Mar 13 2023 11:18:08 GMT+0800","2022-06-05T23:59:35","Observation","Ship Staff","Nav Audit / Verification","LL OFFICERS STRESSED UPON GIVING FEEDBACK TO ALL BRIDGE TEAM MEMBERS ABOUT THEIR FEEDBACK ABOUT THE BRIDGE TEAM PERFORMANCE INCLUDING MASTER'S PERFORMANCE.","Navigation - Others","Navigation","Behaviour Based,Knowledge Based","","","","","AFTER EVERY NAVIGATION OPERATION, BRIDGE TEAM TO EVALUATE AND ASSESS THEIR PEROFORMANCE AND GIVE FEEDBACK TO EACH OTHER IN FRIENDLY ENVIRONMENT IN ORDER TO OVERCOME THE SHORTCOMINGS.","2022-09-05T23:59:35","","Completed","2022-06-05T23:59:35","No","No","No","Internal"]
[null,null,null,30636,42440,"0_Mon Mar 13 2023 11:21:53 GMT+0800","2022-06-05T23:59:35","Other","Ship Staff","Nav Audit / Verification","ALL BRIDGE TEAM MEMBERS EDUCATED AND MADE AWARE OF BLIND SPOT IN THE EYES. BLIND SPOT DETECTION TEST CARRIED OUT WITH ALL BRIDGE TEAM MEMBERS, FOR THEM TO DETECT THE BLIND SPOT IN THEIR EYES.","Navigation - Others","Navigation","Knowledge Based","4.1","High","","","ALL BRIDGE TEAM MEMBERS EDUCATED AND MADE AWARE OF BLIND SPOT IN THE EYES. BLIND SPOT DETECTION TEST CARRIED OUT WITH ALL BRIDGE TEAM MEMBERS, FOR THEM TO DETECT THE BLIND SPOT IN THEIR EYES. ADVISED ALL BRIDGE TEAM MEMBERS TO MAKE THEMSELVES AWARE OF THEIR LIMITATIONS TOO ALONG WITH LIMITATIONS OF NAV AIDS.","2022-09-05T23:59:35","","Completed","2022-06-05T23:59:35","No","No","No","Internal"]
[null,null,null,26629,null,"53_Wed Aug 24 2022 04:39:57 GMT+0000","2022-06-11T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","P & S ACCOMODATION LADDER TO PAINT AND THE SIDE GUARD CHAINS TO DERUST AND PAINT","Deck - Machinery","General Appearance","Equipment Related","11.4","Very High","","","DERUSTING AND PAINTING CARRIED OUT.","2022-09-10T23:59:35","","Completed","2022-08-05T23:59:35","No","No","No","Internal"]
[null,null,null,26425,null,"53_Fri Aug 05 2022 00:58:07 GMT+0000","2022-06-11T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","TUBE LIGHT AND TRANSPARENT COVERS AROUND ACCOMMODATION NEED CLEANING","Elect. Mach. & Equip.","General Appearance","Equipment Related","10.32","Very High","","","COVERS WERE CLEANED OR RENEWED.","2022-07-18T23:59:35","","Completed","2022-07-16T23:59:35","No","No","No","Internal"]
[null,null,null,26428,null,"53_Fri Aug 05 2022 01:11:04 GMT+0000","2022-06-11T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","CONNING DISPLAY, OVERHAETING – SERVICE REQUEST AT SINGAPORE","Navigation - Others","Navigation","Equipment Related","4.3","Medium","","","Service technician attended at Tanjung Bruas on 23-July-2022 and replaced the CCU. Upgraded the software.","2022-08-24T23:59:35","DPUM225042","Completed","2022-07-18T23:59:35","No","No","No","Internal"]
[null,null,null,26429,null,"53_Fri Aug 05 2022 01:13:40 GMT+0000","2022-06-11T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","P & S FWD CHAIN STOPPER RUSTING","Deck - Mooring Machinery","General Appearance","External Factors","11.4","Very High","","","DERUSTING & PAINTING OF SBM STOPPER CARRIED OUT.","2022-09-10T23:59:35","","Completed","2022-07-14T23:59:35","No","No","No","Internal"]
[null,null,null,26430,null,"53_Fri Aug 05 2022 01:15:45 GMT+0000","2022-06-11T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","AIR CON FRESH AIR INTAKE DERUST AND REPAIR","Miscellaneous","General Appearance","Equipment Related","11.4","Very High","","","DERUSTING & PAINTING OF AIRCON FRESH AIR INTAKE GRILL & HOUSING CARRIED OUT","2022-08-10T23:59:35","","Completed","2022-07-13T23:59:35","No","No","No","Internal"]
[null,null,null,26431,null,"53_Fri Aug 05 2022 01:59:40 GMT+0000","2022-06-11T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ALL BUNKER TANK VENTS RUSTING AND ONE OF THEM REQUIRES STEEL RENEWAL STBD FWD OF ACCOMODATION.","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.4","Very High","","","DERUSTING / PAINTING TO BE CARRIED OUT.","2022-08-10T23:59:35","","Completed","2022-07-11T23:59:35","No","No","No","Internal"]
[null,null,null,27233,63440,"53_Thu Sep 01 2022 15:55:09 GMT+0800","2022-06-11T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","PERSONNEL ELEVATOR ER DOOR LATCH TO REPAIR.","Accommodation","General Appearance","Equipment Related,Human Error,Inappropriate Procedure","10.32","Very High","","","Latch to be repaired.","2022-07-10T23:59:35","","Completed","2022-07-23T23:59:35","No","No","No","Internal"]
[null,null,null,25980,80784,"0_Tue Jun 28 2022 21:40:38 GMT+0800","2022-06-11T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","AUS #2 INLET VALVES REPORTED NOT HOLDING WELL","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.34","High","","","OBSERVED THAT DISCHARGE VALVE OP209 IS LEAKING AND CARGO SEEPAGE TO NO.2 COP IS FROM DISCHARGE VALVE.","2022-09-10T23:59:35","","Completed","2023-01-11T23:59:35","No","No","No","Internal","Vessel at CIMC Shipyard (DD) in Zhoushan, China, AUS #2  calibrated and solved."]
[null,null,null,25983,40860,"53_Tue Jun 28 2022 21:47:06 GMT+0800","2022-06-11T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","SEVERAL SUPPORTS AND CABLE PENETRATION PIPES AROUND ACCOMODATION REPAIRS AND DERUST","Accommodation","General Appearance","Equipment Related","11.4","Very High","","","DERUSTING / PAINTING OF D/C/ B DECK COMPLETED\nONLY A DECK AND UPPER DECK REMAINING","2022-09-10T23:59:35","","Completed","2022-11-17T23:59:35","No","No","No","Internal"]
[null,null,null,25984,72006,"53_Wed Jun 29 2022 08:00:42 GMT+0800","2022-06-11T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","CABLE SUPPORT TRAYS AND PIPELINE U-BOLTS ON MAIN DECK TO DERUST AND PAINT","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.4","Very High","","","DERUSTING / PAINTING OF PIPELINE IN PROGRESS - FORWARD OF MANIFOLD.","2022-09-10T23:59:35","","Completed","2022-12-26T23:59:35","No","No","No","Internal","Completed in Shipyard on 30-Dec."]
[null,null,null,25985,61745,"0_Wed Jun 29 2022 08:02:42 GMT+0800","2022-06-11T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","OLD ROPES AND PILOT LADDERS TO DISCARD FROM FORECASTLE","Miscellaneous","General Appearance","External Factors","11.4","Very High","","","SAME TO BE OFFLANDED AT DRY DOCK- SCRUBBER FITTINGS","2022-12-24T23:59:35","","Completed","2022-12-26T23:59:35","No","No","No","Internal","Vessel at CIMC Shipyard (DD) in Zhoushan, China, Offlanding of same is being arranged.\nOfflanded in yard."]
[null,null,null,25987,42649,"0_Wed Jun 29 2022 08:03:45 GMT+0800","2022-06-11T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","PUMP ROOM AIR MUSHROOM AIR FILTER CASING TO REPAIR","Miscellaneous","General Appearance","Equipment Related","11.4","Very High","","","WIRE MESH RENEWED FOR PUMPROOM NATURAL VENT.","2022-09-10T23:59:35","DPUM220210","Completed","2022-07-05T23:59:35","No","No","No","Internal"]
[null,null,null,25991,97533,"53_Tue Jun 28 2022 21:34:01 GMT+0800","2022-06-11T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","PRINTER PAPERS COLLECTOR ROLLER TO MAKE FOR THE WIND MONITOR","Miscellaneous","General Appearance","Equipment Related","8.8","Medium","","","COLLECTOR ROLL MADE & PUT IN USE","2022-07-10T23:59:35","","Completed","2022-06-21T23:59:35","No","No","No","Internal"]
[null,null,null,25992,20849,"0_Tue Jun 28 2022 21:39:07 GMT+0800","2022-06-11T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","PAINT LOCKER TO ARRANGE AND REMOVE EMPTY DRUMS. ","Miscellaneous","General Appearance","Behaviour Based","11.4","Very High","","","PAINT LOCKER ARRANGED","2022-06-16T23:59:35","","Completed","2022-06-11T23:59:35","No","No","No","Internal"]
[null,null,null,25993,82295,"53_Tue Jun 28 2022 21:42:45 GMT+0800","2022-06-11T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","STORAGE SPACE ON THE AFT DECK TO CLEAR UP, SHIFT TUBES AND THE STEEL MATERIAL TO ER","Miscellaneous","General Appearance","Behaviour Based","11.4","Very High","","","TUBES SHIFTED TO STEERING FLAT & SPACE CLEARED","2022-07-10T23:59:35","","Completed","2022-06-20T23:59:35","No","No","No","Internal"]
[null,null,null,25994,42515,"53_Wed Jun 29 2022 08:09:19 GMT+0800","2022-06-11T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","GALLEY STEEL BULKHEADS POLISHING TO BE DONE ","Miscellaneous","General Appearance","Equipment Related","11.4","Very High","","","POLISHING CARRIED OUT FOR GALLEY STEEL BULKHEADS","2022-07-02T23:59:35","","Completed","2022-06-18T23:59:35","No","No","No","Internal"]
[null,null,null,26816,null,"53_Fri Sep 16 2022 04:38:15 GMT+0000","2022-06-11T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","MEAT ROOM INSULATION NEEDS REPAIR","Miscellaneous","MLC Related","Equipment Related","10.32","Very High","","","Repair by shipyard.\nMeat room to be emptied for removal of insulation and inspection of leaking galley drain pipe.\nMeat room ice formation on wall cladding investigation was carried out. All galley dran pipes were inspected, no leak from the drain pipes. There is air ingress through the cladding joints. Repair will be planned in consultation with attending superintendent.","2022-12-24T23:59:35","","Completed","2023-01-06T23:59:35","No","No","No","Internal","Transferred to REFMAN Defect Monitoring for shipyard repair when docking to install ECGS around DEC 2022.\nVessel at CIMC Shipyard (DD) in Zhoushan, China, Same is being attended.\nRectified by Yard."]
[null,null,null,25988,48858,"53_Tue Jun 21 2022 08:33:34 GMT+0800","2022-06-13T23:59:35","Observation,Defect","Others (Eg. Insurance etc.)","ISM Audit","LSHFO SETTLING TANK REMOTE GAUGE MALFUNCTIONING FOR READING","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related,External Factors,Industry Issue","10.32","Very High","","","P/I MODULATOR UNIT TO BE RENEWED.","2022-09-14T23:59:35","DPUM220198","Completed","2022-06-16T23:59:35","No","No","No","External"]
[null,null,null,25974,40763,"53_Tue Jun 21 2022 10:25:16 GMT+0800","2022-06-14T23:59:35","Defect","Others (Eg. Insurance etc.)","ISM Audit","MAIN ENGINE OIL MIST DETECTOR WATER SEPARATOR TO BE INSTALLED AS PER MAKERS ADVISED.","E/R - Main Engine","Eng. / Strg. Comp.","External Factors,Equipment Related,Knowledge Based","10.32","Very High","","","WATER SEPARATOR TO BE INSTALLED IN AIR LINE.","2022-09-14T23:59:35","DPUM220199","Completed","2022-06-28T23:59:35","No","No","No","External"]
[null,null,null,25975,88490,"53_Thu Jun 23 2022 19:42:42 GMT+0800","2022-06-14T23:59:35","Observation,Defect","Others (Eg. Insurance etc.)","ISM Audit","ME UNIT #5 AFT FUEL VALVE LEAKING FROM COLLAR – TO REPLACE","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related,Human Error,Knowledge Based","10.32","Very High","","","FUEL VALVE TO BE RENEWED.","2022-07-08T23:59:35","","Completed","2022-06-28T23:59:35","No","No","No","External"]
[null,null,null,25976,87579,"0_Thu Jun 23 2022 19:44:16 GMT+0800","2022-06-14T23:59:35","Observation","Others (Eg. Insurance etc.)","ISM Audit","MAIN ENGINE  HPU MINOR LEAK FROM PLUG WASHER","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related,External Factors,Inappropriate Procedure","10.32","Very High","","","WASHER TO BE RENEWED.","2022-07-08T23:59:35","","Completed","2022-06-28T23:59:35","No","No","No","External"]
[null,null,null,25989,69705,"53_Fri Jun 24 2022 08:26:23 GMT+0800","2022-06-14T23:59:35","Observation","Others (Eg. Insurance etc.)","ISM Audit","PORT AUX BLR LOWER SIGHT GLASS SLIGHTLY DIRTY, CLEANING REQUIRED","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related,External Factors,Inappropriate Procedure,Human Error","10.32","Very High","","","SIGHT GLASS TO BE CLEANED.","2022-06-17T23:59:35","","Completed","2022-06-17T23:59:35","No","No","No","External"]
[null,null,null,25995,27366,"0_Thu Jun 23 2022 19:46:36 GMT+0800","2022-06-14T23:59:35","Observation","Others (Eg. Insurance etc.)","ISM Audit","MAIN ENGINE JACKET WATER OUTLET LINE AUTO VENT ONE PLUG HAS SIGN OF LEAKS AND CORROSION – TO OVERHAUL","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related,External Factors,Inappropriate Procedure","10.32","Very High","","","CLEANED AND RENEWED.","2022-07-14T23:59:35","","Completed","2022-06-21T23:59:35","No","No","No","External"]
[null,null,null,26642,null,"53_Thu Sep 01 2022 04:14:05 GMT+0000","2022-06-24T23:59:35","Defect","Ship Staff","Ship Staff Insp.","During Routine Inspection of No.2 BWTS filter found 2 Number of Candle filter damaged,","Miscellaneous","Cargo / Ballast Systems","Equipment Related","8.8","Medium","","","Damaged filter candles renewed with new filter candles received under PO# DPUM220209. BWTS Tested after renewal of filter candles and found working satisfactory.","2022-09-24T23:59:35","DPUM220209","Completed","2022-08-19T23:59:35","No","No","No","Internal"]
[null,null,null,26424,null,"53_Fri Aug 05 2022 00:54:34 GMT+0000","2022-07-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","It was observed that the port Anchor flukes are not resting on hawse pipe lips when anchor is stowed & secured in position.","Deck - Mooring Machinery","Mooring","Equipment Related","9.2","Very High","","","Twist on the port anchor chain flukes removed as per the procedures provided by the office staff.","2022-09-30T23:59:35","","Completed","2022-07-21T23:59:35","No","No","No","Internal"]
[null,null,null,26423,null,"53_Fri Aug 05 2022 00:52:32 GMT+0000","2022-07-03T23:59:35","Defect","Ship Staff","Ship Staff Insp.","BWTS Plant main ballast line FCV 1121 Positioner Malfunctioning.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related,External Factors,Industry Issue","6.21","High","","","As per makers instruction calibration carried out, need to be renewed positioner.","2022-10-04T23:59:35","DPUM220218","Completed","2022-07-21T23:59:35","No","No","No","Internal"]
[null,null,null,26422,null,"53_Fri Aug 05 2022 00:48:51 GMT+0000","2022-07-09T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Hose Handling Crane personnel transfer winch limit switch malfunctioning for up direction.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.50","Medium","","","Block Disassembled and noticed pitting marks on piston and dent on the body, need to be renewed complete block. Waiting for makers advise to identify correct part numbers. Spare received & fitted. OK now.","2022-10-09T23:59:35","DPUM220229","Completed","2022-07-21T23:59:35","No","No","No","Internal"]
[null,null,null,26420,null,"53_Thu Aug 04 2022 10:22:47 GMT+0000","2022-07-15T23:59:35","Defect","Ship Staff","Ship Staff Insp.","\"Found 4S Cow machine valve has a crack on its Body &\n3P : No.1 COW machine valve spindle sheared off.\n\"","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.34","High","","","COW machine valve to be renewed.","2022-10-14T23:59:35","DPUM220256","Completed","2022-09-29T23:59:35","No","No","No","Internal","PO# DPUM220256 delivered onboard on the 5th SEP 2022 at SINGAPORE. Revert rectification."]
[null,null,null,27231,60582,"53_Fri Jul 22 2022 13:00:22 GMT+0800","2022-07-15T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Found 4S Cow machine valve has a crack on its Body &\n3P : No.1 COW machine valve spindle sheared off.\n","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.34","High","","","REPLACED COW VALVES FOR 4S AND 3P.","2022-10-14T23:59:35","DPUM220235","Completed","2022-09-13T23:59:35","No","No","No","Internal"]
[null,null,null,26628,null,"53_Wed Aug 24 2022 04:18:50 GMT+0000","2022-08-05T23:59:35","Defect","Ship Staff","Ship Staff Insp.","ECR ALARM STROBE LAMP NOT WORKING","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","JOB ORDER NO. :V-DPUM041856/22\nECR strobe light was replaced with new spare received.","2022-11-05T23:59:35","DPUM220264","Completed","2022-12-23T23:59:35","No","No","No","Internal","PO# DPUM220264 issued to OCEAN MARINE. Waiting for spare readiness."]
[null,null,null,27230,24347,"53_Thu Aug 25 2022 00:01:57 GMT+0800","2022-08-17T23:59:35","Observation","Ship Staff","Ship Staff Insp.","OUTER LAYER OF BOTH LIFEBOATS AIR CYLINDER HOSE CONNECTING TO THE MANIFOLD FOUND DAMAGED. NO LEAKAGE OBSERVED. ","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.29","High","","","Both life boats air cylinders hoses replaced with new spare. Hose specification: K-OCEAN, SIZE: 3/8\"X2W, Working pressure 33.0 MPa. Life Boat No.1 501.002.00.01 JO DPUM042386/22 & Life Boat No.2 501.002.00.02 JO DPUM042387/22. ","2022-11-16T23:59:35","DPUM220252","Completed","2022-09-29T23:59:35","No","No","No","Internal"]
[null,null,null,27232,39339,"53_Wed Aug 24 2022 23:42:13 GMT+0800","2022-08-17T23:59:35","Observation","Ship Staff","Ship Staff Insp.","BOTH LIFEBOAT TRIGGER WIRES ( LASHING WIRES) FOUND RUSTED,  FEW WIRE STRANDS ARE DAMAGED. ","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.29","High","","","RENEWED GRIPES FOR BOTH LIFEBOATS","2022-11-16T23:59:35","DPUM220252","Completed","2022-09-22T23:59:35","No","No","No","Internal"]
[null,null,null,27218,35119,"53_Mon Aug 29 2022 10:37:51 GMT+0800","2022-08-23T23:59:35","Defect","Ship Staff","Ship Staff Insp.","BALLAST WATER TREATMENT PLANT MAIN BALLAST BOTH LINE MAIN FILTER BACK-FLUSHING MOTOR RUNNING CONTINUOUSLY.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related,External Factors,Industry Issue","6.21","High","","","MAKERS INFORMED AND AWAITING  SUGGESTION FOR PROXIMITY SENSOR OR EPROM PROGRAM. THIS NEEDS FURTHER INVESTIGATION AFTER CLEANING FILTER ELEMENTS. \nBWTS UPGRADED WILL BE DONE AS NON-FILTER TYPE. Being closed as job re- raised in 2023","2022-12-30T23:59:35","DPUM220259","Completed","2022-12-29T23:59:35","No","No","Yes","Internal","Do advise on the present status of the issue."]
[null,null,null,26812,null,"53_Fri Sep 16 2022 04:07:21 GMT+0000","2022-08-25T23:59:35","Defect","Ship Staff","Ship Staff Insp.","OWS Discharge Line vent valve is slightly leaking for water during operation.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Leaking vent valve renewed with new spare, tried out working satisfactory.\nJob Order no :- 803.025.00.00//V-DPUM043354/22","2022-11-24T23:59:35","DPUM220273","Completed","2022-11-13T23:59:35","No","No","No","Internal","PO# DPUM220273 issued to Korean maker GEORIM. Spare readiness about 13th SEP 2022."]
[null,null,null,27220,16516,"53_Fri Sep 09 2022 08:11:04 GMT+0800","2022-08-30T23:59:35","Defect","Ship Staff","Ship Staff Insp.","HIGH SEA CHEST FILTER IN LINE RUBBER COATING ARE IN DAMAGED CONDITION","","Eng. / Strg. Comp.","Equipment Related,External Factors,Industry Issue","10.32","Very High","","","PRESENTLY DAMAGED SECTION CUT AND RENEWED WITH NEW RUBBER.2-3 COAT OF EPOXY PAINTED ON SURFACE,THE JOB SCOPE HAS TRANSFERRED TO REFMAN.\n.AS PER SUPERINTENDENT RUDDER COATING REPAIR NOT BE CARRIED OUT THIS CALL DD.COMPLETED NEW FILTER CASING WILL BE INSTALLED ON NEXT DRY DOCKING.\t","2022-12-04T23:59:35","","Completed","2022-12-27T23:59:35","No","No","No","Internal"]
[null,null,null,26814,null,"53_Fri Sep 16 2022 04:16:50 GMT+0000","2022-08-30T23:59:35","Defect","Ship Staff","Ship Staff Insp.","\"vessel received an “ zone 11 HC 3 IR blocked” alarm on Accm gas detection display in CCR. and locally on detector head display we noticed “F-02” & “F-03” alarm respectively. Suspecting Detector malfunctioning and to be renewed.\n\"","Accommodation","Safety / LSA / FFA","Behaviour Based","8.46","Very High","","","RECEIVED SPARE AND RENEWED","2022-11-29T23:59:35","DPUM220277","Completed","2022-12-27T23:59:35","No","No","No","Internal","PO# DPUM220277 issued to HONEYWELL. Waiting spare readiness."]
[null,null,null,27226,60461,"0_Fri Sep 30 2022 18:10:14 GMT+0800","2022-08-31T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Deck foam system sea water flushing valve was found not holding, during deck foam pump routine trying out.\n","Critical Equip.","Emgcy. Systems","Equipment Related","5.35","Medium","","","Deck foam system sea water flushing valve replaced with new scew down glove valve 16K50.\n\nSystem tested and verified that the new valve holding.\n\nUnplanned job DPUM042195/22 is updated and necessary documents attached. \n","2022-09-23T23:59:35","","Completed","2022-09-21T23:59:35","No","No","No","Internal"]
[null,null,null,26815,null,"53_Fri Sep 16 2022 04:20:23 GMT+0000","2022-09-02T23:59:35","Defect","Ship Staff","Ship Staff Insp.","HOSE HANDLING CRANE PORT SIDE TANK EMERGENCY QUICK COUPLING CONNECTION IS RUSTED CONDITION.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.50","Medium","","","Leaking Emergency quick coupling with new spare, tried out working satisfactory.\nJob Order no:- 383.001.00.01//V-DPUM043355/22","2022-12-02T23:59:35","DPUM220282","Completed","2022-11-13T23:59:35","No","No","No","Internal","PO# DPUM220282 issued to NCS. Waiting spare readiness."]
[null,null,null,27227,97432,"0_Fri Sep 30 2022 18:13:27 GMT+0800","2022-09-17T23:59:35","Defect","Ship Staff","Ship Staff Insp.","AE No.3 Lo priming pump power supply unit faulty.Pump fail to start auto or in manual.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","power supply unit renewed with yard supply spare and pump tried out working satisfactory.","2022-09-23T23:59:35","","Completed","2022-09-19T23:59:35","No","No","No","Internal"]
[null,null,null,27225,70471,"53_Fri Sep 30 2022 18:00:44 GMT+0800","2022-09-19T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Air cooler end cover gasket leaking and AE no. 2 trip on high HT temperature.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Air cooler removed from place and gasket renewed with fabricated onboard. Air cooler pressure tested to 7.5 bar found satisfactory. Air cooler installed back in place tried out working satisfactory.","2022-09-20T23:59:35","","Completed","2022-09-19T23:59:35","No","No","No","Internal"]
[null,null,null,27228,64169,"53_Sat Oct 08 2022 21:53:15 GMT+0800","2022-09-25T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Fire and G.S Pump no.1 leak thru mech.seal","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.35","Very High","","","Pump isolated and overhauling carried out with new spare mech seal.pump tried out working satisfactory.tested up to 12 bar.","2022-09-27T23:59:35","","Completed","2022-09-26T23:59:35","No","No","No","Internal"]
[null,null,null,27229,95478,"0_Sat Oct 08 2022 21:58:56 GMT+0800","2022-09-27T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Main fire pump no.1 and 2 delivery hard to close ( struck in open position).","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.35","Very High","","","valve eased up after loosening gland.found rusted and same cleared.tried out working satisfactory. ","2022-10-01T23:59:35","","Completed","2022-09-27T23:59:35","No","No","No","Internal"]
[null,null,null,30637,87103,"0_Mon Mar 13 2023 11:25:54 GMT+0800","2022-09-29T23:59:35","Observation","Ship Staff","Nav Audit / Verification","No Compass error was recorded in compass error log after large alteration of course.","Navigation - Others,Documentation","Navigation","Human Error,Knowledge Based","4.9","Medium","","","All officers briefed on to take error upon large alteration of course and during navigational watch. During change of watch (At Sea) relieving officer to verify that error being recorded after large alteration of course in previous watch.","2022-12-29T23:59:35","","Completed","2022-10-25T23:59:35","No","No","No","Internal"]
[null,null,null,30638,33161,"0_Mon Mar 13 2023 11:29:12 GMT+0800","2022-09-29T23:59:35","Defect","Ship Staff","Nav Audit / Verification","Auto telephone handset wire PVC coating found in damaged condition on both bridge wing panels.","Navigation - GMDSS & Communication","Navigation","Equipment Related","4.7","High","","","Auto telephone Handset wire to be changed with new one. Inspection of all auto & Sound powered telephone and its accessories to be carried out on regular basis. Any defect found, same to be reported as soon as possible.","2022-12-29T23:59:35","","Completed","2022-10-25T23:59:35","No","No","No","Internal"]
[null,null,null,30639,79376,"53_Mon Mar 13 2023 13:16:33 GMT+0800","2022-09-29T23:59:35","Observation","Ship Staff","Nav Audit / Verification","Position and time for hand steering tried out not mentioned in deck logbook.","Documentation,Navigation - Others","Navigation","Human Error","4.10","High","","","ALL OFFICERS BRIEFED ON TO MAKE MAKE HAND STEERING ENTRY IN DECK LOG BOOK REMARKS SECTION WITH POSITION AND TIME OF ACTUAL TRY OUT.","2022-12-29T23:59:35","","Completed","2022-10-25T23:59:35","No","No","No","Internal"]
[null,null,null,30644,62843,"0_Mon Mar 13 2023 13:19:29 GMT+0800","2022-09-29T23:59:35","Observation","Ship Staff","Nav Audit / Verification","Signature of radio personnel & times in which radio watch commences / ends to be recorded in the GMDSS logbook","Documentation,Navigation - GMDSS & Communication","Navigation","Human Error,Knowledge Based","4.23","High","","","Signature of radio personnel & times in which radio watch commences / ends trecorded in the GMDSS logbook after briefing to officers.","2022-12-29T23:59:35","","Completed","2022-10-25T23:59:35","No","No","No","Internal"]
[null,null,null,30645,67888,"0_Mon Mar 13 2023 13:21:33 GMT+0800","2022-09-29T23:59:35","Defect","Ship Staff","Nav Audit / Verification","Dimmer for Clinometer not functioning properly, same to be attended","Navigation - Others","Navigation","Equipment Related","4.7","High","","","Dimmer & dimmer switch to be inspected and change if required.  All officers to be briefed on If any abnormality is observed same to be reported as soon as possible.","2022-12-29T23:59:35","","Completed","2023-10-25T23:59:35","No","No","No","Internal"]
[null,null,null,27389,58754,"53_Wed Oct 19 2022 00:12:50 GMT+0800","2022-10-11T23:59:35","Defect","Ship Staff","Ship Staff Insp.","LOW SEA CHEST FILTER IN LINE RUBBER COATING ARE IN DAMAGED CONDITION","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related,External Factors,Industry Issue","10.32","Very High","","","RUBBER COAT OR LINING NEED TO BE RENEWED/REPAIRED IN THE UPCOMING DRY DOCK (EGCS INSTALLATION).AS PER SUPERINTENDENT RUDDER COATING REPAIR NOT BE CARRIED OUT THIS CALL DD.COMPLETED NEW FILTER CASING WILL BE INSTALLED ON NEXT DRY DOCKING.\n","2022-12-23T23:59:35","","Completed","2022-12-27T23:59:35","No","No","No","Internal"]
[null,null,null,27390,73274,"53_Fri Oct 28 2022 16:14:20 GMT+0800","2022-10-11T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","Bottom step of pilot ladder damaged at PSVM terminal .","Deck - Machinery","Safety / LSA / FFA","External Factors","5.47","Medium","","","Replaced with new ladder","2022-12-24T23:59:35","DPUM220310","Completed","2022-11-18T23:59:35","No","No","No","Internal"]
[null,null,null,27687,82428,"53_Fri Nov 04 2022 17:43:49 GMT+0800","2022-10-25T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Main air compressor no.1 and 2 air leak from cooler high pressure side (seal ring damage).","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Leak rectified and compressor tested found satisfactory.\nJob order MAC No.1: 731.001.06.01//V-DPUM043352/22  \nJob order MAC No.2: 731.001.06.02//V-DPUM043353/22  \n","2022-11-30T23:59:35","DPUM220160","Completed","2022-11-11T23:59:35","No","No","No","Internal"]
[null,null,null,30696,35508,"53_Tue Jan 31 2023 17:06:32 GMT+0800","2023-01-28T23:59:35","Guarantee Claim","Ship Staff","Ship Staff Insp.","During Sea trial, 3-way Solenoid valve (S0V00402) inside CEMS cabinet is to select sample or ambient air malfunction. Same removed from place, dismantled and checked. Hair line cracks inside solenoid valve body. To be renewed.  ","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Temporary repair was carried out in presence of attending service engineer. New spare received. Same installed & in use.","2023-03-12T23:59:35","GC001/23","Completed","2023-03-18T23:59:35","No","No","No","Internal"]
[null,null,null,30726,82627,"53_Fri Feb 10 2023 00:02:28 GMT+0800","2023-01-29T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","cleaning and painting of funnel","Miscellaneous","General Appearance","Equipment Related","11.2","Medium","","","funnel stacks scraped and  painted with HT back. Rest of the funnel in good condition","2023-04-28T23:59:35","","Completed","2023-04-13T23:59:35","No","No","No","Internal"]
[null,null,null,30571,94425,"53_Thu Feb 09 2023 16:41:29 GMT+0800","2023-01-29T23:59:35","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Main deck pipelines clamp observed to  be rusted.","Deck - Pipe / Fittings","General Appearance","External Factors","11.4","Very High","","","Main deck pipelines clamp derusting and painting completed.","2023-08-14T23:59:35","","Completed","2023-08-13T23:59:35","No","No","No","Internal",""]
[null,null,null,30607,91985,"0_Thu Feb 09 2023 16:49:06 GMT+0800","2023-01-29T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Stores in midship , accommodation and forecastle requires cleaning and arranging.","Accommodation","","Inappropriate Procedure","11.12","Low","","","All stores midship , forecastle and accomodation cleaned and arranged","2023-02-07T23:59:35","","Completed","2023-02-06T23:59:35","No","No","No","Internal"]
[null,null,null,30608,79384,"0_Thu Feb 09 2023 16:53:58 GMT+0800","2023-01-29T23:59:35","Critical Equipment","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Fore peak eductor not taking suction.Drive line for same to be modified.","Deck - Pipe / Fittings","Safety / LSA / FFA","Equipment Related","5.1","Very High","","","Drive line for fore peak eductor modified  .Eductor tried out and taking good suction.","2023-02-07T23:59:35","","Completed","2023-01-31T23:59:35","No","No","No","Internal"]
[null,null,null,30609,47112,"53_Mon Feb 13 2023 13:25:36 GMT+0800","2023-01-29T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Mess room chairs observed to be dirty and stains in dry dock.","Accommodation","General Appearance","Equipment Related","11.1","High","","","All mess room chairs sop washed and sun dried.","2023-02-25T23:59:35","","Completed","2023-02-02T23:59:35","No","No","No","Internal"]
[null,null,null,30616,24201,"0_Wed Feb 22 2023 17:31:43 GMT+0800","2023-01-29T23:59:35","Observation","Ship Staff","Ship Staff Insp.","ECR Telephone buttons found malfunctioning. ","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Same renewed with onboard spare.","2023-05-12T23:59:35","","Completed","2023-01-29T23:59:35","No","No","No","Internal"]
[null,null,null,30625,82376,"53_Mon Feb 13 2023 13:22:35 GMT+0800","2023-01-29T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Bunker vend heads in china passgae cover plates thinned down and wasted.","Miscellaneous","Structural Condn. / WT integrity ","Equipment Related","11.1","High","","","Wasted and thinned plates removed & new ones fabricated in E/R workshop. Same installed.","2023-03-28T23:59:35","NA","Completed","2023-02-24T23:59:35","No","No","No","Internal"]
[null,null,null,30650,97101,"0_Mon Feb 13 2023 13:27:05 GMT+0800","2023-01-29T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Swimming pool area to clean and shower head missing.","Accommodation","General Appearance","Equipment Related","11.1","High","","","Swimming pool area cleaned, derusting and painting carried out , final coat painted.",null,"","Completed","2023-03-04T23:59:35","No","No","No","Internal"]
[null,null,null,30618,32379,"0_Wed Feb 22 2023 17:29:39 GMT+0800","2023-02-02T23:59:35","Observation","Ship Staff","Ship Staff Insp.","HFO Settling Tank Transfer Pump Cut-In Float not actuating. ","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Same opened up. Float found with heavy carbon/fuel deposits. Cleaned & re-installed. Tried out & found in order.","2023-05-12T23:59:35","NA","Completed","2023-02-07T23:59:35","No","No","No","Internal"]
[null,null,null,30619,39347,"0_Wed Feb 22 2023 17:22:08 GMT+0800","2023-02-03T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Shaft Earthing Showing value more than 80mV. ","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.38","Medium","","","Found the shaft & band with rust. Same removed & bands re-installed. In use & in order.","2023-05-03T23:59:35","NA","Completed","2023-02-10T23:59:35","No","No","No","Internal"]
[null,null,null,30610,57904,"53_Thu Feb 16 2023 19:37:05 GMT+0800","2023-02-08T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Port & Stbd Windlass Bow Stopper found sluggish & hard to operate by hand.Require chain blocks to open and close. Same to be freed up & greased appropriately.","Deck - Mooring Machinery","Mooring","Equipment Related","9.20","Medium","","","Both anchor bow stopper  pawl was removed. Turned the shaft using Mooring winch 10-12 times using Counter weight and then Counter weight was removed and Shaft was made free by moving Pulling out on either side. Grooving for the pin was buffed and cleaned lubricated for free movement. Full assembly of roller type chain stopper boxed back and tried out .Presently bow stopper can be smoothly lifted and placed in position.","2023-02-22T23:59:35","","Completed","2023-02-15T23:59:35","No","No","No","Internal"]
[null,null,null,30617,65783,"0_Wed Feb 22 2023 17:51:07 GMT+0800","2023-02-09T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Both Hose Handling Cranes Emcy Stop Levers found corroded & one handle broke during operation. ","Deck - Machinery","Emgcy. Systems","Equipment Related","8.50","Medium","","","Both replaced with new onboard spares. RO will be raised for consumed spares.","2023-05-12T23:59:35","","Completed","2023-02-11T23:59:35","No","No","No","Internal"]
[null,null,null,30727,16104,"0_Wed Feb 22 2023 17:46:53 GMT+0800","2023-02-12T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Port & Stbd Hose Handling Cranes main block operating levers are hard to operate and do not return to neutral position. ","Deck - Machinery","General Appearance","Equipment Related","8.50","Medium","","","Levers freed  and same noticed to be free and normal during loading operation at Porto Do Acu.","2023-05-12T23:59:35","","Completed","2023-04-23T23:59:35","No","No","No","Internal"]
[null,null,null,30743,66211,"0_Wed Feb 22 2023 19:30:23 GMT+0800","2023-02-12T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Incinerator ash door safety lock air cylinder is found defective. ","E/R - Aux. Mach.","MARPOL Related","Equipment Related","10.32","Very High","","","RO DPUM230033 raised. Spare received on 31-May-2023. Same renewed & tried out. In order.","2023-05-12T23:59:35","RO DPUM230033","Completed","2023-05-31T23:59:35","No","No","No","Internal"]
[null,null,null,30744,42402,"0_Wed Feb 22 2023 19:27:16 GMT+0800","2023-02-12T23:59:35","Observation","Ship Staff","Ship Staff Insp.","ER Blower #4 Flap 3-way valve also found corroded. ","Critical Equip.","Emgcy. Systems","Equipment Related","5.45","Medium","","","Replacement required. RO DPUM230069 Raised  for new spares. Renewed with spares received at Singapore on 31-May-2023","2023-05-12T23:59:35","RO DPUM230069","Completed","2023-06-01T23:59:35","No","No","No","Internal"]
[null,null,null,30745,23085,"0_Wed Feb 22 2023 19:22:27 GMT+0800","2023-02-12T23:59:35","Observation","Ship Staff","Ship Staff Insp.","IG Platform Oxygen Sensor #1 found unable to calibrate to O2 20.9. ","Critical Equip.","Emgcy. Systems","Equipment Related","8.30","High","","","Suspect detector head sensor defective. raised RO DPUM230072 for new sensors heads. Both sensors renewed with new received spares at Singapore on 31-May-2023. Tried out & in order.","2023-05-12T23:59:35","DPUM230072","Completed","2023-05-29T23:59:35","No","No","No","Internal"]
[null,null,null,30746,65307,"0_Wed Feb 22 2023 17:37:45 GMT+0800","2023-02-12T23:59:35","Observation","Ship Staff","Ship Staff Insp.","It is observed that the MSB 220V insulation frequently received from Radar UPS & VSAT Antenna. Radar ","Navigation - RADAR","Emgcy. Systems","Equipment Related","10.38","Medium","","","RO DPUM230039 raised. Received spare at Singapore on 31-May-2023. System in use.","2023-05-12T23:59:35","DPUM230039","Completed","2023-05-29T23:59:35","No","No","No","Internal"]
[null,null,null,30569,42065,"0_Wed Feb 22 2023 17:33:33 GMT+0800","2023-02-12T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Wheelhouse Telephone buttons worn out/malfunctioning & need replacement.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","RO DPUM230048 raised for spare. buttons renewed. All damaged telephone handset cords that were damaged have been renewed.","2023-07-14T23:59:35","RO DPUM230048","Completed","2023-07-12T23:59:35","No","No","No","Internal","DPUM230048 - to be supplied soonest"]
[null,null,null,30570,46332,"0_Wed Feb 22 2023 17:52:42 GMT+0800","2023-02-12T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Various Deck Pipelines & support brackets found corroded  Also Cable gaurds corroded and holed","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","11.5","Medium","","","Various Deck Pipelines & support brackets de-rusted & checked. Renew by clamping if required as no hotwork can be done on deck..Derusting and temp renewal in progress.same to be added to DD list for permanent repairs.","2023-08-14T23:59:35","","Completed","2023-08-13T23:59:35","No","No","No","Internal","Noted in Progress"]
[null,null,null,30575,99555,"0_Wed Feb 22 2023 17:42:55 GMT+0800","2023-02-12T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Deck pipelines especially HFO & LSMGO Bunker filling lines found rusted at various locations.","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.4","Very High","","","HFO & LSMGO Bunker filling lines wasted Sections have been removed & repaired with new section of pipes in the Workshop. Derusting and painting carried out on required section of line. Cosmetic upgradation completed.\n","2023-05-12T23:59:35","NA","Completed","2023-05-21T23:59:35","No","No","No","Internal","Please confirm if all completed, then the same is to be closed."]
[null,null,null,30577,62870,"0_Wed Feb 22 2023 19:28:16 GMT+0800","2023-02-12T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Engine room signal light columns (12 in number) electric horns are found defective/not working.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","RO DPUM230030 raised & received. Rectification in progress. 8 pcs defective horns renewed. All signal columns found working now.","2023-05-12T23:59:35","DPUM230030","Completed","2023-06-29T23:59:35","No","No","No","Internal","Please advise if all completed."]
[null,null,null,30581,87606,"53_Thu Feb 23 2023 17:55:28 GMT+0800","2023-02-12T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Main BWTS FCV found unable to regulate flow when both ballast pumps are running.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","6.21","High","","","Found an air leak in the FCV controller. Rectified. System tried out & found regulating satisfactorily.","2023-06-01T23:59:35","NA","Completed","2023-05-31T23:59:35","No","No","No","Internal","Noted that vessel has found an air leak in the FCV controller and same was rectified. S\n\nIf system is regulating satisfactorily, then this defect can be closed."]
[null,null,null,30611,19145,"0_Wed Feb 22 2023 17:56:39 GMT+0800","2023-02-12T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Sanitary Fan Wire Meshes found choked. ","Accommodation","General Appearance","Equipment Related","5.10","High","","","Same removed, cleaned & boxed back. Sanitary fan suction in Accommodation is satisfactory.","2023-05-12T23:59:35","NA","Completed","2023-02-18T23:59:35","No","No","No","Internal"]
[null,null,null,30612,49713,"0_Wed Feb 22 2023 17:59:43 GMT+0800","2023-02-12T23:59:35","Observation","Ship Staff","Ship Staff Insp.","EGCS Sea Water Pump #1 Discharge Line flange found with pinhole leak by way of the flange weld seam. ","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.31","Very High","","","Elbow removed & repaired by welding in the Workshop. Re-installed & tried out. In order.","2023-05-12T23:59:35","NA","Completed","2023-02-14T23:59:35","No","No","No","Internal"]
[null,null,null,30613,92899,"0_Wed Feb 22 2023 19:21:08 GMT+0800","2023-02-12T23:59:35","Observation","Ship Staff","Ship Staff Insp.","EGCS System found not tripping after activation of ES-A & CO2 Trip. ","Critical Equip.","Emgcy. Systems","External Factors","10.32","Very High","","","Found the ES-A & CO2 trip connected in Parallel. Same connected in series & found in order.","2023-05-12T23:59:35","NA","Completed","2023-02-10T23:59:35","No","No","No","Internal"]
[null,null,null,30614,22970,"0_Wed Feb 22 2023 19:26:29 GMT+0800","2023-02-12T23:59:35","Observation","Ship Staff","Ship Staff Insp.","ER Blower #3 Flap 3-Way Valve found corroded. Handle broke during operation. ","Critical Equip.","Emgcy. Systems","Equipment Related","5.45","Medium","","","3-way valve swapped with Purifier room damper 3-way valve. Valve temporarily repaired & installed on the Purifier room damper. RO to be raised for spare.","2023-05-14T23:59:35","","Completed","2023-02-14T23:59:35","No","No","No","Internal"]
[null,null,null,30615,65670,"53_Wed Feb 22 2023 19:19:08 GMT+0800","2023-02-12T23:59:35","Observation","Ship Staff","Ship Staff Insp.","EGCS Ovbd Valves Indication lamps for Open/Shut found swapped. ","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","External Factors","10.32","Very High","","","Indication lamps swapped. Now showing correctly.","2023-05-12T23:59:35","NA","Completed","2023-02-11T23:59:35","No","No","No","Internal"]
[null,null,null,30620,63963,"0_Wed Feb 22 2023 17:15:57 GMT+0800","2023-02-12T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Composite Boiler Feed Water Pump #2 starter found showing “Abnormal” during running.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Pump Stby-Start Pressure transmitter found malfunctioning. Same renewed with new onboard spare. RO raised for consumed spare.","2023-05-12T23:59:35","","Completed","2023-02-15T23:59:35","No","No","No","Internal"]
[null,null,null,30621,13304,"0_Wed Feb 22 2023 19:29:15 GMT+0800","2023-02-12T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Emcy Fire Pump found not building sufficient pressure in the Fire Line. ","Critical Equip.","Emgcy. Systems","Equipment Related","10.32","Very High","","","Priming Device checked & found stuck. Same freed up. Pump tried out & operating satisfactorily.","2023-05-12T23:59:35","NA","Completed","2023-02-13T23:59:35","No","No","No","Internal"]
[null,null,null,30626,30353,"0_Wed Feb 22 2023 17:28:20 GMT+0800","2023-02-12T23:59:35","Observation","Ship Staff","Ship Staff Insp."," Bunker Tank #2(P) Remote & Local Level gauge not working & showing zero. ","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","\"Dual check safety chamber\" and \"Pneumatic modulator\" dismantled and cleaned.","2023-05-12T23:59:35","","Completed","2023-02-21T23:59:35","No","No","No","Internal"]
[null,null,null,30630,36680,"53_Wed Feb 22 2023 17:13:28 GMT+0800","2023-02-12T23:59:35","Observation","Ship Staff","Ship Staff Insp.","ME FO Circulating Pump #2 found vibrating during operation.","E/R - Pumps","","Equipment Related","10.32","Very High","","","Pump overhauled. Found the bearing damaged. Same renewed with new spare. Boxed up & tried out. In order. RO raised for consumed spares.","2023-05-12T23:59:35","","Completed","2023-02-22T23:59:35","No","No","No","Internal"]
[null,null,null,30631,39215,"0_Wed Feb 22 2023 17:27:36 GMT+0800","2023-02-12T23:59:35","Observation","Ship Staff","Ship Staff Insp.","HFO Settling Tank Remote & Local Level Gauge found not working & showing zero.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","\"Dual check safety chamber\" and \"Pneumatic modulator\" dismantled and cleaned.","2023-05-12T23:59:35","","Completed","2023-02-23T23:59:35","No","No","No","Internal"]
[null,null,null,30652,21757,"0_Wed Feb 22 2023 17:26:01 GMT+0800","2023-02-12T23:59:35","Observation","Ship Staff","Ship Staff Insp.","LSHFO Service Tank Remote & Local level gauge not matching manual sounding. The gauge is showing less than the actual sounding. ","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","I/P converter has been overhauled. Tank filled up & gauge is operating. Values matching now.","2023-05-12T23:59:35","NA","Completed","2023-03-09T23:59:35","No","No","No","Internal"]
[null,null,null,30694,24220,"0_Wed Feb 22 2023 17:38:57 GMT+0800","2023-02-12T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Steering Gear #1 Port side Ram leaking from the Seal. ","Critical Equip.","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Same nipped up. Leak has reduced to about 100ml/day. Under observation. No leak observed apart from the regular lubrication.","2023-05-12T23:59:35","NA","Completed","2023-03-28T23:59:35","No","No","No","Internal"]
[null,null,null,30695,93990,"0_Wed Feb 22 2023 17:24:29 GMT+0800","2023-02-12T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Bunker tanks No.1 (S) Remote level gauge is not matching manual sounding. Local gauge is in order. The gauge is showing more than the actual sounding.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","I/P converter has been overhauled. Tank qty verified after bunkering. IN use & operating satisfactorily.","2023-05-12T23:59:35","NA","Completed","2023-03-18T23:59:35","No","No","No","Internal"]
[null,null,null,30701,69582,"0_Wed Feb 22 2023 19:31:38 GMT+0800","2023-02-12T23:59:35","Observation","Ship Staff","Ship Staff Insp.","During bunkering it was noted that on forward side both port and stbd HFO manifold valves are not holding as manifold pressure gauges were showing positive pressure with valves fully shut. Bunker manifold valves to be replaced. Also forward-stbd bunker manifold valve actuator is not in place and instead a handle is fitted to operate the valve. ","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.4","Very High","","","Spare valves received. All Bunker Manifold Valve valves renewed with new received spares. ","2023-05-12T23:59:35","DPUM230036","Completed","2023-04-09T23:59:35","No","No","No","Internal"]
[null,null,null,30702,24873,"0_Wed Feb 22 2023 17:54:55 GMT+0800","2023-02-12T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Bridge Telegraph lever is not matching the displayed value on the monitor. ","Navigation - Others","Navigation","Equipment Related","4.7","High","","","Calibration carried out. In order.","2023-05-12T23:59:35","NA","Completed","2023-04-11T23:59:35","No","No","No","Internal"]
[null,null,null,30704,34283,"0_Wed Feb 22 2023 17:53:54 GMT+0800","2023-02-12T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Bridge Wing Units (Port & Stbd) Telegraph levers found not matching the display. ","Navigation - Others","Navigation","Equipment Related","4.7","High","","","Calibration carried out. In order.","2023-05-12T23:59:35","NA","Completed","2023-04-11T23:59:35","No","No","No","Internal"]
[null,null,null,30715,99633,"0_Wed Feb 22 2023 17:44:05 GMT+0800","2023-02-12T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Drinking Water Fountain in Steering Gear room body & fittings are corroded. To be replaced with new. RO DPUM230035 raised.","Miscellaneous","MLC Related","Equipment Related","10.32","Very High","","","Fountain replaced with new received spare. In use.","2023-05-12T23:59:35","DPUM230035","Completed","2023-04-19T23:59:35","No","No","No","Internal"]
[null,null,null,30633,58869,"0_Tue Feb 28 2023 01:32:23 GMT+0800","2023-02-17T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Anchor WIndlass (Stbd) found with leak by way of the control lever spindle.","Deck - Mooring Machinery","Mooring","Equipment Related","9.2","Very High","","","Control lever block overhauled & new o-rings & seals installed. Windlass tried out & found operating satisfactorily with no leaks.","2023-05-17T23:59:35","NA","Completed","2023-02-20T23:59:35","No","No","No","Internal"]
[null,null,null,30622,15566,"53_Tue Feb 28 2023 01:20:51 GMT+0800","2023-02-21T23:59:35","Observation","Ship Staff","Ship Staff Insp.","ME Fuel Oil Circulating Pump #2 found with abnormal sound during operation.\n\n","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Pump Bearing found seized & not moving freely. Same renewed with new spare. Pump tried out & found in order.","2023-05-21T23:59:35","NA","Completed","2023-02-22T23:59:35","No","No","No","Internal"]
[null,null,null,30623,85336,"0_Tue Feb 28 2023 01:23:01 GMT+0800","2023-02-21T23:59:35","Observation","Ship Staff","Ship Staff Insp.","ME Fuel Oil Circulating Pump #2 Motor found with cold repair on the brackets.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Same renewed with new onboard spare. Tried out & in use.","2023-05-21T23:59:35","NA","Completed","2023-02-22T23:59:35","No","No","No","Internal"]
[null,null,null,30624,50870,"0_Tue Feb 28 2023 01:35:28 GMT+0800","2023-02-21T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Anchor Windlass (Port) Clutch hydraulic lever found seized & not moving freely. The lever broke during operation.","Deck - Mooring Machinery","Mooring","Equipment Related","9.20","Medium","","","Same removed & lever renewed. Block overhauled & new orings & seals installed in the spindle. Tried out & operating satisfactorily.","2023-05-21T23:59:35","NA","Completed","2023-02-22T23:59:35","No","No","No","Internal"]
[null,null,null,30584,34643,"0_Tue Feb 28 2023 01:27:14 GMT+0800","2023-02-23T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Observed The HFO Purifier #1 Supply Pump operating with abnormal sound & leaking from the coupling area.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Pump stopped & opened up for inspection. Found the pump bearing damaged with parts broken away. Also noticed the magnetic coupling casing is damaged. The bearing has been renewed. Coupling casing has been cold repaired & installed. Pump tried out & operating satisfactorily. RO raised DPUM230068 for consumed spares & new magnetic coupling.supply of spares awaited. P/P is tried out and running satisfactory.","2023-08-20T23:59:35","RO DPUM230068","Completed","2023-08-20T23:59:35","No","No","No","Internal","Noted that Pump tried out & operating satisfactorily.  Then this defect can be closed.\n\nRO raised DPUM230068 for consumed spares & new magnetic coupling to be supplied to the vessel soonest."]
[null,null,null,30647,22392,"53_Tue Feb 28 2023 01:43:48 GMT+0800","2023-02-23T23:59:35","Observation","Ship Staff","Ship Staff Insp.","EGCS alarms received “WMS-002 Sampling Water flow low alarm” & \"WMP-002 Pump Stop”.\n","E/R - Main Engine,E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Found the WMS-002 Pump leaking. The pump was opened up for inspection. Found the pump diaphragm damaged & the motor also seized due to water ingress. RO DPUM230063 & GC-004 raised for new pump with motor. Pump renewed with new received spare & in use. No leaks observed.","2023-05-23T23:59:35","RO DPUM230063 & GC-004","Completed","2023-03-08T23:59:35","No","No","No","Internal"]
[null,null,null,30734,67542,"0_Mon May 15 2023 19:57:46 GMT+0800","2023-03-03T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Aft Hydraulics SW Cooler Inlet Pipelines found with pinhole & seepage leaks at various places.","Deck - Mooring Machinery,Deck - Pipe / Fittings","Mooring","Equipment Related","9.14","Medium","","","Complet pipe sections (4 in nos.) removed & brought to workshop. Fabricated complete new pipes. Same installed & tried out. No leaks","2023-08-03T23:59:35","NA","Completed","2023-05-12T23:59:35","No","No","No","Internal"]
[null,null,null,30649,94377,"0_Wed Mar 15 2023 11:04:19 GMT+0800","2023-03-03T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Lifeboat #2, found with Diesel oil near the bottom plug.","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","Noticed the Fuel Tank Return line Flexible hose damaged at the connection due to getting brittle.The remaining hose was checked & found in order & not brittle. The damaged section was cropped & the hose reinstalled. The estimated qty of diesel leaked is about 18ltrs. The fuel tank has been topped up. The engine has been tried out & confirmed no leaks. \nLifeboat #1(Stbd) was also checked & hose found in order. \nThe hose was also cropped & reinstalled.","2023-06-03T23:59:35","NA","Completed","2023-03-03T23:59:35","No","No","No","Internal"]
[null,null,null,30670,12317,"53_Wed Mar 15 2023 10:58:56 GMT+0800","2023-03-03T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Lifeboat #1 & #2 Sprinkler System Spider Coupling found fabricated onboard out of Teflon. ","LSA / FFA","Safety / LSA / FFA","Equipment Related","8.69","Medium","","","Spares under RO DPUM230081 received. Spider Couplings renewed for both Lifeboats with new received spares.","2023-06-03T23:59:35","DPUM230081","Completed","2023-03-26T23:59:35","No","No","No","Internal"]
[null,null,null,30641,75371,"0_Wed Mar 15 2023 11:09:26 GMT+0800","2023-03-05T23:59:35","Observation","Ship Staff","Ship Staff Insp.","During Changeover to LSMGO, ME & AE Backwash Filters found leaking from the shaft.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Seals for both filters renewed. Tried out & in use.","2023-06-05T23:59:35","NA","Completed","2023-03-03T23:59:35","No","No","No","Internal"]
[null,null,null,30742,75633,"53_Wed Mar 15 2023 15:51:15 GMT+0800","2023-03-06T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Gas Detection System found with minor leaks.","Critical Equip.","Safety / LSA / FFA","Equipment Related","8.30","High","","","Banjo Connectors damaged. RO DPUM230076 raised. \n9 Nos. Banjo connectors renewed with new spare on 30-Mar-2023. Remaining leaking connectors with new spares received at Singapore on 31-May-2023. System tried out & in use. No leaks observed.","2023-06-06T23:59:35","DPUM230076","Completed","2023-05-29T23:59:35","No","No","No","Internal"]
[null,null,null,30642,19583,"0_Wed Mar 15 2023 11:13:00 GMT+0800","2023-03-06T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Aux. Boiler #1 Atomizing steam Inlet Bonnet found leaking. ","E/R - Pipes/ valves & fittings,E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","bonnet gasket renewed. Tried out & in order.","2023-06-07T23:59:35","NA","Completed","2023-03-08T23:59:35","No","No","No","Internal"]
[null,null,null,30643,67210,"0_Wed Mar 15 2023 11:18:16 GMT+0800","2023-03-07T23:59:35","Observation","Ship Staff","Ship Staff Insp.","BWTS TRO Sensor Sampling & Washing Water Lines choked.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","6.21","High","","","Both Lines manually cleared. SOlenoid valves found completely choked & rusted stuck in closed position. Same renewed with new onboard spares. System tried out & lines clear.","2023-06-07T23:59:35","NA","Completed","2023-03-07T23:59:35","No","No","No","Internal"]
[null,null,null,30648,79688,"53_Wed Mar 15 2023 11:27:58 GMT+0800","2023-03-07T23:59:35","Observation","Ship Staff","Ship Staff Insp.","COP #1 Master trip activated in CCR panel.","Cargo Mach.,Elect. Mach. & Equip.","Cargo / Ballast Systems","Equipment Related","6.21","High","","","On checking, found the trip only showing on the CCR panel & able to operate the COP. Found #A-CC-W6 cable #5 break. same replaced with spare cable #15. Tried out the trips & found in order.","2023-06-07T23:59:35","NA","Completed","2023-03-11T23:59:35","No","No","No","Internal"]
[null,null,null,30646,52625,"0_Wed Mar 15 2023 11:20:20 GMT+0800","2023-03-08T23:59:35","Observation","Ship Staff","Ship Staff Insp.","ME ECS UPS-B power supply unit #T105 found malfunctioning. ","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","\nFound \"DC OK\" and \"BOOST\" LED flickering.\nThe Output voltage checked found fluctuating. Unit #T105 was replaced with Spare Unit #T112. System tried out &  found in order.","2023-06-08T23:59:35","NA","Completed","2023-03-08T23:59:35","No","No","No","Internal"]
[null,null,null,30587,84348,"53_Fri Mar 31 2023 20:43:22 GMT+0800","2023-03-13T23:59:35","Observation","Ship Staff","Ship Staff Insp.","ME SFF Filter (Bypass Unit) found giving differential alarm.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","As the vessel had only Only 2 pcs filters onboard, two elements renewed with new spare on 27-Mar-2023. Filter unit put back online. No spare onboard. RO DPUM230031 raised.. Spares received. no alarm now.","2023-06-13T23:59:35","DPUM230031","Completed","2023-05-30T23:59:35","No","No","No","Internal","If ME SFF Filter ( by pass unit) alarm issue is resolved - then, this Defect can be closed.  RO DPUM230031 - should be on board by now."]
[null,null,null,30689,19219,"53_Fri Mar 31 2023 19:56:34 GMT+0800","2023-03-13T23:59:35","Observation","Ship Staff","Ship Staff Insp.","AE #2 Jacket Cooling Water Pressure found low.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","On investigation found the Air Cooler leaking by way of the end cover. The end cover was renewed with shore fabricated spare. The fabricated end cover found 5mm thicker than the original cover. Same ground & installed. AE tried out & found in order.","2023-06-13T23:59:35","NA","Completed","2023-03-13T23:59:35","No","No","No","Internal"]
[null,null,null,30690,90194,"0_Fri Mar 31 2023 19:58:31 GMT+0800","2023-03-13T23:59:35","Observation","Ship Staff","Ship Staff Insp.","ME Jacket Water Heater Steam Inlet Valve found with pinhole leak from the body.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Valve renewed with new spare. Tried out & found in order.","2023-06-13T23:59:35","NA","Completed","2023-03-13T23:59:35","No","No","No","Internal"]
[null,null,null,30691,58488,"0_Fri Mar 31 2023 20:00:00 GMT+0800","2023-03-13T23:59:35","Observation","Ship Staff","Ship Staff Insp.","AE #2 Crankcase Door Relief Valve found leaking.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","o-ring found brittle. Same renewed. AE in use.","2023-06-18T23:59:35","NA","Completed","2023-03-18T23:59:35","No","No","No","Internal"]
[null,null,null,30735,97275,"53_Thu Mar 30 2023 19:36:46 GMT+0800","2023-03-14T23:59:35","Observation","Owner / Marine / Tech. Suptd.","ISM Audit","M/E Cylinder Oil 3x1000 litres containers found kept on C-Deck Starboard Side. Same to be transferred to designated tank at the earliest opportunity.","Miscellaneous","General Appearance","Equipment Related","","","","","Cubitainers contents transferred to the Cyl Oil Storr Tank #1 & ME LO Settl Tank in order to blend with the present oil TBN. Cubitainers lashed & stored on C-Deck iteslf as per advise from Technical.","2023-06-12T23:59:35","NA","Completed","2023-04-30T23:59:35","No","No","No","Internal"]
[null,null,null,30585,40378,"53_Sat Mar 25 2023 17:44:48 GMT+0800","2023-03-14T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Pipelines - Rust spots found to be just painted over on the pipelines all acr0ss the vessel. Very poor surface preparation.","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","Inappropriate Procedure","11.4","Very High","","","Hydroballasting, derusting & painting of deck pipelines is in progress..Vessel completed derusting and painting up to no-7 foam monitor till 01.05.2023","2023-07-28T23:59:35","","Completed","2023-07-28T23:59:35","No","No","No","Internal","Noted in progress"]
[null,null,null,30592,26986,"53_Mon May 01 2023 06:17:20 GMT+0800","2023-03-14T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Mooring winch - Brake band for few mooring winches found very uneven. Please send a separate mail to Technical wrt this.","Deck - Mooring Machinery","Mooring","Equipment Related","9.14","Medium","","","Brake band of all mooring winches derusting, painting and brake padding renewal carried out.","2023-07-28T23:59:35","DPUM 230094-MOORING WINCH BRAKE LINING","Completed","2023-07-30T23:59:35","No","No","No","Internal","Please confirm the remaining 6 brake bands ic completed now."]
[null,null,null,30654,32239,"53_Sat Mar 25 2023 09:06:50 GMT+0800","2023-03-14T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Bunkering Audit","ISPS - Securing bar for ISPS in the accomodation is not solving the purpose. ","Accommodation","ISPS Related","Behaviour Based","4.4","High","","","All Accomodation Doors  are provided with bars for securing arrangements to lock them from inside. During inspation time the locking bar was not used  properly. Same has been rectified and all the Bars were checked and inserted peoperly. All crew members were briefed for how to use the bar properly. ","2023-03-27T23:59:35","","Completed","2023-03-20T23:59:35","No","No","No","Internal"]
[null,null,null,30655,27170,"53_Sat Mar 25 2023 09:16:26 GMT+0800","2023-03-14T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Bunkering Audit","During bunker operation Upper deck weather tight doors kept full open","Accommodation","Safety / LSA / FFA","Behaviour Based","5.1","Very High","","","Immedietely Door closed & all other doors & SIP checked & verified that all are closed. later on  All officers & Crew were briefed about the right procedure that at port or at anchor whenever there is cargo or bunker operations is going on, keep all the SIP & accomodations doors closed. Only one access door  (opposite to berth) designate for in & out. All duty personnal were advised for the same & to report to duty officers.","2023-03-28T23:59:35","","Completed","2023-03-18T23:59:35","No","No","No","Internal"]
[null,null,null,30656,29858,"53_Sat Mar 25 2023 09:22:35 GMT+0800","2023-03-14T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Bunkering Audit","House keeping of the mid ship locker should be improved. Found dirty","Accommodation","General Appearance","Behaviour Based","11.1","High","","","All stores are arranged properly. All loose items secured propely in place. All crew were briefed to mainatin the cleaniness inside th accomadation & stores. Do not store the garbage inside the stores. & don't put any thing in the way of safety equipments.","2023-03-27T23:59:35","","Completed","2023-03-20T23:59:35","No","No","No","Internal"]
[null,null,null,30657,54394,"53_Sat Mar 25 2023 09:40:06 GMT+0800","2023-03-14T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Bunkering Audit","Mooring Pipeline - M4 mooring winch remote operating pipeline found leakign from the coupling. Understand from shipstaff that this issue has been ongoing since quiet some time without any permanent rectification. ","Deck - Mooring Machinery","Mooring","External Factors","11.4","Very High","","","Pipe were slacken from both the ends & then retightened from both the ends. Now the leak has stopped. same was also tested by running the winch. During testing no leak was observed. Still that pipe is under observation for any leak.\nAll crew members were instructed to take good rounds & report if they see any thing abnormal.","2023-03-27T23:59:35","","Completed","2023-03-18T23:59:35","No","No","No","Internal"]
[null,null,null,30659,80213,"53_Fri Mar 24 2023 19:39:45 GMT+0800","2023-03-14T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Bunkering Audit","Water Ballast Pump - WBP no 2 suction gauge in the CCR found to have completely turned and showing out of range pressure. Discharge pressure also showing very high. To be checked and calibrated if required. ","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.13","Medium","","","Zero callibration for all pressure guages for Ballast & Cargo pumps carried out, now both Locally & CCR are showing the same reading. During the inspaection on ballast side there was actual pressure due to that presuure was showing high. Later on after operating the valve pressure become normal & and gauges were showing the correct reading. ","2023-03-22T23:59:35","","Completed","2023-03-20T23:59:35","No","No","No","Internal"]
[null,null,null,30660,78400,"53_Sat Mar 25 2023 09:43:47 GMT+0800","2023-03-14T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Bunkering Audit","Chemical drums found stored in the VRCS room. What is the purpose of these drums in the VRCS room? IS this for refilling of VRCS tank? ","Accommodation","General Appearance","Behaviour Based","11.1","High","","","Chemical drums have been removed from VRCS rooms. All crew members were briefed not to store anything inside the vrcs room.","2023-03-28T23:59:35","","Completed","2023-03-16T23:59:35","No","No","No","Internal"]
[null,null,null,30661,59537,"53_Sat Mar 25 2023 09:56:33 GMT+0800","2023-03-14T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Smoking room - Dustbin for ash found half full. This should be emptied on regualr basis ","Accommodation","Safety / LSA / FFA","Behaviour Based","11.13","Low","","","Bin  emptied after putting the ash into another bin & kept it for some time to avoid the chance of fire . Same was briefed to crew members to clear the bins on regular daily basis with proper segrigation","2023-03-17T23:59:35","Smoking room - Dustbin for ash found half full. This should be emptied on regualr basis ","Completed","2023-03-15T23:59:35","No","No","No","Internal"]
[null,null,null,30662,58186,"53_Sat Mar 25 2023 10:11:20 GMT+0800","2023-03-14T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Dryer Room - Boiler suits found hanging on the electrical cables and conduits  & Dryer room - Lint not removed from dryers in the laundry","Miscellaneous","General Appearance","Behaviour Based","11.14","Medium","","","All clothes which were hanging removed from Laundary. All dryer filters cleaned.\n All crew members were advised not to hang any clothes on the electrical cables or anywhere inside the laundary or alleways. All filters shall be clean after use. As it may cause a fire inside the laundary.","2023-03-15T23:59:35","","Completed","2023-03-15T23:59:35","No","No","No","Internal"]
[null,null,null,30663,89922,"53_Sat Mar 25 2023 10:23:14 GMT+0800","2023-03-14T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Life jackets in the Midship store found without Ships name","LSA / FFA","ISM Related","Inappropriate Procedure","5.32","High","","","All Life jackets & life west checked. wherever the ship's name & port of registry missing same were stenciled on them. ","2023-03-22T23:59:35","","Completed","2023-03-18T23:59:35","No","No","No","Internal"]
[null,null,null,30664,12484,"53_Sat Mar 25 2023 17:11:29 GMT+0800","2023-03-14T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Chemicals - MSDS for few chemicals in the Midship locker and Chemical locker found outdated. New MSDS to be downloaed from the internet and replaced with latest ones. ","Miscellaneous","ISM Related","Human Error","5.46","Medium","","","Latest MSDS downloaded & same were posted in designated areas","2023-03-22T23:59:35","","Completed","2023-03-22T23:59:35","No","No","No","Internal"]
[null,null,null,30665,30708,"53_Sat Mar 25 2023 17:57:52 GMT+0800","2023-03-14T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Cargo Manifold - Starboard manifold grating iwo vapour manifold found not properly secured and loose. ","Hull & Tanks","MARPOL Related","External Factors","6.6","Medium","","","Loose Grating on stbd side manifold properly secured with J-hooks.\nManifold drip tray grating on both side checked for any missing J-hook all are in place & properly secured.","2023-03-22T23:59:35","","Completed","2023-03-22T23:59:35","No","No","No","Internal"]
[null,null,null,30666,78887,"53_Sat Mar 25 2023 18:12:07 GMT+0800","2023-03-14T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Life raft - Life cradle to be derusted and painted. ","LSA / FFA","Safety / LSA / FFA","Human Error,External Factors","5.30","High","","","All life raft cradles derusted & painted.","2023-03-22T23:59:35","","Completed","2023-03-18T23:59:35","No","No","No","Internal"]
[null,null,null,30667,34360,"53_Sat Mar 25 2023 10:27:55 GMT+0800","2023-03-14T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Lifting equipment - Few Chain blocks in the mid ship locker found safety latch damaged. ","Miscellaneous","ISM Related","External Factors","8.50","Medium","","","All chain blocks latchs were repaired & locking hook satisfactorly.","2023-04-07T23:59:35","","Completed","2023-03-22T23:59:35","No","No","No","Internal"]
[null,null,null,30668,39480,"53_Tue Mar 28 2023 21:14:04 GMT+0800","2023-03-14T23:59:35","Other,Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Pipelines - Bunker line pressure testing dates from stenciled at few places.\n","Deck - Pipe / Fittings","General Appearance","Human Error","","","","","Stenciling carried out on Bunker pipelines mentioning the last pressure tested dates on port and stbd side bunker manifold lines and common line of bunker manifold.","2023-06-13T23:59:35","","Completed","2023-03-18T23:59:35","No","No","No","Internal"]
[null,null,null,30669,42655,"53_Sat Mar 25 2023 10:01:48 GMT+0800","2023-03-14T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","VRCS room - Oil leak observed in the VRCS pump save all ","Deck - Machinery","Cargo / Ballast Systems","Behaviour Based","11.4","Very High","","","Savall cleaned & very minor leak detected fro rubber hose coupling same was tightned & leak was rectified.","2023-03-27T23:59:35","","Completed","2023-03-15T23:59:35","No","No","No","Internal"]
[null,null,null,30671,71555,"0_Thu Mar 30 2023 19:15:54 GMT+0800","2023-03-14T23:59:35","Non Conformity","Owner / Marine / Tech. Suptd.","ISM Audit","Windlass gear was not found greased for both Port & Starboard Sides.","Deck - Mooring Machinery","General Appearance","Human Error","","","","","Greasing of Windlass gears carried out.","2023-06-12T23:59:35","NA","Completed","2023-03-15T23:59:35","No","No","No","Internal"]
[null,null,null,30672,64887,"0_Thu Mar 30 2023 19:17:59 GMT+0800","2023-03-14T23:59:35","Non Conformity","Owner / Marine / Tech. Suptd.","ISM Audit","Insulation meter at Forward Bosun Store appears malfunctioning. Upon depressing the Test Button, Phase T blacks out but the needle deflection is minimal.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","Circuit checked & rectified. Fwd Insulation meter is in order.","2023-06-12T23:59:35","NA","Completed","2023-03-16T23:59:35","No","No","No","Internal"]
[null,null,null,30673,63074,"53_Thu Mar 30 2023 19:32:41 GMT+0800","2023-03-14T23:59:35","Observation","Owner / Marine / Tech. Suptd.","ISM Audit","Latest Tracking Sheet under IHM saved in File Management System is dated 16 Nov 2022.","Documentation","Cert. & Docu.","Human Error","","","","","Last tracking sheet received on 12-Jan-2023 & same updated in FMS. Latest Tracking sheet updated in FMS on 23-Mar-2023.","2023-06-12T23:59:35","NA","Completed","2023-03-20T23:59:35","No","No","No","Internal"]
[null,null,null,30674,60659,"53_Thu Mar 30 2023 19:38:48 GMT+0800","2023-03-14T23:59:35","Observation","Owner / Marine / Tech. Suptd.","ISM Audit","1. Expired ISO 9001 and ISO 14001 displayed in Ship’s Office.\n2. Obsolete version of Initial Notification SOPEP FORM being used on board. Current version of Form to be replaced at all locations.","Documentation","Cert. & Docu.","Human Error","","","","","1.ISO 9001& ISO 14001 Replaced with latest ones. 2.Initial notification form inserted in all locations ","2023-06-12T23:59:35","NA","Completed","2023-03-14T23:59:35","No","No","No","Internal"]
[null,null,null,30675,93134,"0_Thu Mar 30 2023 19:46:02 GMT+0800","2023-03-14T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ME Cylinder Oil daily tank - Gauge glass found gagged. \n","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Human Error","","","","","ME Cylinder Oil daily tank Gauge glass gagging tool removed and briefing carried out for all E/R Staff and explained the consequences for the same. ","2023-06-13T23:59:35","","Completed","2023-03-15T23:59:35","No","No","No","Internal"]
[null,null,null,30676,16792,"53_Fri Mar 31 2023 16:02:00 GMT+0800","2023-03-14T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Pipeline - HFO 1P bunker tank inlet valve found very hard. To be eased up and greased","Deck - Pipe / Fittings","MARPOL Related","Equipment Related","","","","","Valve freed up & greased. All other valves also tried out & greased.","2023-06-12T23:59:35","NA","Completed","2023-03-18T23:59:35","No","No","No","Internal"]
[null,null,null,30677,71948,"53_Thu Mar 30 2023 19:13:05 GMT+0800","2023-03-14T23:59:35","Non Conformity","Owner / Marine / Tech. Suptd.","ISM Audit","SCBA Compressor relief valves are rated 225 and 330 bars. Lifeboat Air Bottles filling pressure is 140 bars and it is noted that SCBA compressor is used to top up the L/B air bottles.","Critical Equip.","Emgcy. Systems","Inappropriate Procedure","","","","","Procedure verified and posted near BA Compressor. Training carried out for all Personnel.","2023-06-12T23:59:35","NA","Completed","2023-03-15T23:59:35","No","No","No","Internal",""]
[null,null,null,30678,61366,"0_Thu Mar 30 2023 19:43:18 GMT+0800","2023-03-14T23:59:35","Non Conformity","Owner / Marine / Tech. Suptd.","MLC Audit","Strong foul smell from AB Cabin toilet, adjacent to Shop’s Office. Same to be trouble shoot and resolve. Weekly inspection of accommodation to be strengthened.    ","Accommodation","MLC Related","Inappropriate Procedure","","","","","During inspection it was found that smell was coming from Toilet drain. Immediately drain was cleaned with hot water, Now no more smell is coming from drain. During meeting messman & other crew members involved in cleaning were instructed to clean the drain in common areas & cabins on regular basis","2023-06-12T23:59:35","NA","Completed","2023-03-17T23:59:35","No","No","No","Internal"]
[null,null,null,30679,57220,"0_Thu Mar 30 2023 19:41:50 GMT+0800","2023-03-14T23:59:35","Non Conformity","Owner / Marine / Tech. Suptd.","ISPS Audit","Port anchor was in use but the hawse pipe cover was not secured.","Deck - Mooring Machinery","ISPS Related","Human Error","","","","","All officers & deck crew were briefed & instructed to make sure after anchoring hawse pipe cover must be properly secured.","2023-06-12T23:59:35","NA","Completed","2023-03-17T23:59:35","No","No","No","Internal"]
[null,null,null,30680,93983,"0_Thu Mar 30 2023 19:40:23 GMT+0800","2023-03-14T23:59:35","Observation","Owner / Marine / Tech. Suptd.","ISM Audit","Earthing wire of Starboard L/B winch motor found broken/disconnected.","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","Earthing cable installed. Other Earthing cables also checked & found in order.","2023-06-12T23:59:35","NA","Completed","2023-03-20T23:59:35","No","No","No","Internal"]
[null,null,null,30681,58015,"53_Fri Mar 31 2023 16:05:13 GMT+0800","2023-03-14T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Pump room bulkhead in way of COPs in the Engine room found very dirty and needs to be cleaned. ","Miscellaneous","Eng. / Strg. Comp.","","","","","","Bulkhead cleaned & painted.","2023-06-14T23:59:35","NA","Completed","2023-03-18T23:59:35","No","No","No","Internal"]
[null,null,null,30682,51332,"0_Fri Mar 31 2023 16:07:09 GMT+0800","2023-03-14T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Emergency Fire pump suction valve remote operating handle found not stencilled ","E/R - Pipes/ valves & fittings","Emgcy. Systems","Inappropriate Procedure","","","","","Stenciling carried out.","2023-06-14T23:59:35","NA","Completed","2023-03-20T23:59:35","No","No","No","Internal"]
[null,null,null,30683,88065,"0_Fri Mar 31 2023 16:09:05 GMT+0800","2023-03-14T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","EGCS Bilge alarm - To be stencilled ","E/R - Pipes/ valves & fittings","Emgcy. Systems","Inappropriate Procedure","","","","","Stenciling carried out.","2023-06-14T23:59:35","NA","Completed","2023-03-19T23:59:35","No","No","No","Internal"]
[null,null,null,30684,35585,"53_Thu Mar 30 2023 19:42:05 GMT+0800","2023-03-14T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Hydraulic bracing for the Main Engines found heavily rusted. \n","E/R - Main Engine","General Appearance","Equipment Related","","","","","Hydraulic top bracing for main engine  de-rusted and cleaned.","2023-06-13T23:59:35","","Completed","2023-03-20T23:59:35","No","No","No","Internal"]
[null,null,null,30685,64093,"0_Fri Mar 31 2023 16:13:26 GMT+0800","2023-03-14T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Forward stern tube seal - Forward stern tube seal pressure gauge not working - Please check the system thoroughly ","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Pressure gauge faulty. Same renewed.","2023-06-14T23:59:35","NA","Completed","2023-03-20T23:59:35","No","No","No","Internal"]
[null,null,null,30686,63705,"0_Fri Mar 31 2023 16:20:53 GMT+0800","2023-03-14T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","IG Deck seal pump - Leak observed from the flange and complete tray found in dirty condition. All leaks to be rectified, cleaned and painted. ","Inert Gas","Eng. / Strg. Comp.","Inappropriate Procedure","10.32","Very High","","","No leaks observed. Area cleaned & painted.","2023-06-14T23:59:35","NA","Completed","2023-03-18T23:59:35","No","No","No","Internal"]
[null,null,null,30687,36727,"0_Fri Mar 31 2023 16:23:44 GMT+0800","2023-03-14T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Logbook - Main engine details entered incorrectly. To be corrected and updated ","Miscellaneous","Cert. & Docu.","Knowledge Based","","","","","Main Engine Details verified & found in order.","2023-06-14T23:59:35","NA","Completed","2023-03-17T23:59:35","No","No","No","Internal"]
[null,null,null,30688,26972,"0_Fri Mar 31 2023 16:24:51 GMT+0800","2023-03-14T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ECR - COCOS computer found hanging and unable to access due to slow speed. Troubleshooting to carried out in consultation with makers. ","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","COCOS computer operating satisfactorily after following maker instructions.","2023-06-14T23:59:35","NA","Completed","2023-03-22T23:59:35","No","No","No","Internal"]
[null,null,null,30697,27747,"0_Fri Mar 31 2023 16:26:23 GMT+0800","2023-03-14T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Starboard HHC - Safety latch for Personnel lifting hook found damaged. To be rectified. ","Deck - Machinery","Cargo / Ballast Systems","Equipment Related","","","","","BOTH HHC HOOKS LATCH (FOR MANNED HANDLING HOOKS & MAIN HOOKS) FREED, GREASED & REPAIRED.","2023-06-14T23:59:35","","Completed","2023-04-04T23:59:35","No","No","No","Internal"]
[null,null,null,30698,87897,"53_Sat Mar 25 2023 17:21:16 GMT+0800","2023-03-14T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Mooring Winch - Few Mooring winches oil found emulsified. To be inspected and CA to be taken. ","Deck - Mooring Machinery","Mooring","Equipment Related","9.14","Medium","","","Cleaning Of Sight Glass And Emulsified Hydraulic Oil Renewed For  Winches  M6, M5, M3,M2,M1,Wm1 &Wm2 Mooring Winches. M7,M8 & M4 Winch's Oil Is Checked & Found Still In Good Condition.","2023-05-07T23:59:35","","Completed","2023-04-08T23:59:35","No","No","No","Internal"]
[null,null,null,30700,26608,"0_Fri Mar 31 2023 16:14:35 GMT+0800","2023-03-14T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Main Engine Air cooler drain gauge sight glass found dirty","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Sight glasses cleaned. ","2023-06-14T23:59:35","NA","Completed","2023-04-11T23:59:35","No","No","No","Internal"]
[null,null,null,30713,46992,"53_Sat Mar 25 2023 18:04:25 GMT+0800","2023-03-14T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Manifold reducers - Vapour manifold reducer in the midship area found rusted. Needs to be derusted and stored properly. ","Deck - Pipe / Fittings","General Appearance","External Factors,Human Error","11.4","Very High","","","Pipeline derusting & painting is completed.","2023-05-07T23:59:35","NA","Completed","2023-04-11T23:59:35","No","No","No","Internal"]
[null,null,null,30651,50258,"53_Tue Mar 21 2023 17:32:05 GMT+0800","2023-03-16T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Bunkering Audit","Gas Sampling system - Both panels In the CCR for gas sampling showing different timings. All timings to be synchonised. \nPR - 1146 hrs\nWBT - 1824 hrs\nAccom - Also different","Critical Equip.","Safety / LSA / FFA","Equipment Related","5.21","Medium","","","Both the panel corrected for date and time in UTC. now both rae showing corrcet date & time","2023-03-18T23:59:35","","Completed","2023-03-18T23:59:35","No","No","No","Internal"]
[null,null,null,30653,58492,"53_Tue Mar 21 2023 18:02:58 GMT+0800","2023-03-17T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Bunkering Audit","ISPS - Securing bar for ISPS in the accomodation is not solving the purpose. ","Accommodation","ISPS Related","Behaviour Based","7.4","Low","","","All Securing bar checked for all the accomodation doors. Bars are available for all the doors and are properly locking the doors from inside.","2023-03-22T23:59:35","","Completed","2023-03-18T23:59:35","No","No","No","Internal"]
[null,null,null,30658,62890,"53_Tue Mar 21 2023 17:29:07 GMT+0800","2023-03-18T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Bunkering Audit","Gas sampling system failure alarm active. Fault to be identified and rectified. ","Critical Equip.","Safety / LSA / FFA","Equipment Related","5.21","Medium","","","Faulty alarm for ballast tank & pump room gas detaction system already rectified & now there is no faulty alarm on pannel  a& system is working satisfactory.","2023-04-27T23:59:35","","Completed","2023-03-20T23:59:35","No","No","No","Internal"]
[null,null,null,30692,62279,"0_Fri Mar 31 2023 20:02:31 GMT+0800","2023-03-18T23:59:35","Observation","Ship Staff","Ship Staff Insp.","AE #1 Air Cooler End Cover Leak","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","The end cover was renewed with shore fabricated spare. The fabricated end cover found 5mm thicker than the original cover. Same ground & installed. AE tried out & found in order","2023-06-18T23:59:35","NA","Completed","2023-03-18T23:59:35","No","No","No","Internal"]
[null,null,null,30693,67454,"53_Fri Mar 31 2023 20:05:49 GMT+0800","2023-03-18T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Aft Hydraulics Cooler SW Inlet line leaking.","Deck - Mooring Machinery","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Found the line with a pinhole leak. Same rectified by welding. Installed back & tried out. In order.","2023-06-18T23:59:35","NA","Completed","2023-03-20T23:59:35","No","No","No","Internal"]
[null,null,null,30712,75967,"0_Sun Apr 16 2023 02:59:58 GMT+0800","2023-03-24T23:59:35","Observation","Ship Staff","Ship Staff Insp.","ME Unit #7 Exhaust Valve Positioner Sensor Values are erratic.\nME Slow Down activated due to this.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Sensor renewed with new onboard spare. Same tried out & found in order.","2023-06-24T23:59:35","NA","Completed","2023-04-11T23:59:35","No","No","No","Internal"]
[null,null,null,30703,86401,"53_Fri Mar 31 2023 20:50:10 GMT+0800","2023-03-25T23:59:35","Observation","Ship Staff","Ship Staff Insp.","FWG Deflector dislodged & brackets broken.\n","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","The FWG was stopped & Sight glass opened up for inspection.\nFound the Evaporator Deflector Plate dislodged & the brackets damaged. Clamp & bracket arrangement fabricated. Installed & tried out. FWG in use.","2023-06-25T23:59:35","NA","Completed","2023-03-30T23:59:35","No","No","No","Internal"]
[null,null,null,30699,53979,"0_Fri Mar 31 2023 20:55:34 GMT+0800","2023-03-28T23:59:35","Observation","Ship Staff","Ship Staff Insp.","ME Jacket Water Temperature Controller found unable to regulate temperature.","E/R - Main Engine,Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","The positioner found malfunctioning. Same renewed with onboard new spare. Controller tried out & in use. Performing satisfactorily.",null,"NA","Completed","2023-03-28T23:59:35","No","No","No","Internal"]
[null,null,null,30739,25413,"53_Sun Apr 16 2023 03:15:51 GMT+0800","2023-03-29T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Wheelhouse Window Wiper #7 not operating.\nThis only operates when the system is initially switched on.\nAfter one complete cycle, this wiper stops operating.\nIt does not operate when switched on individually.","Navigation - Others","Navigation","Equipment Related","","","","","The trouble was traced to the parking (proximity) sensor. No spare available onboard.. RO “DPUM230075 – Window Wiper Parking Sensor” raised for the same. Spare received & replaced. Wiper tried out & operating satisfactorily. ","2023-06-28T23:59:35","DPUM230075","Completed","2023-05-29T23:59:35","No","No","No","Internal"]
[null,null,null,30705,99152,"53_Sun Apr 16 2023 01:37:09 GMT+0800","2023-03-29T23:59:35","Observation","Ship Staff","Ship Staff Insp.","FWG SW Inlet Line Pressure Gauge Stub Piece Pin Hole leak.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Same repaired by welding. Rectified.","2023-06-28T23:59:35","NA","Completed","2023-03-29T23:59:35","No","No","No","Internal"]
[null,null,null,30706,21895,"0_Sun Apr 16 2023 01:40:53 GMT+0800","2023-03-29T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Jacket Water Controller Temperature found Fluctuating.","E/R - Pipes/ valves & fittings,Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Positioner found malfunctioning. Same renewed with onboard new spare. Tried out & in order. ","2023-06-28T23:59:35","NA","Completed","2023-03-29T23:59:35","No","No","No","Internal"]
[null,null,null,30722,49898,"53_Sun Apr 16 2023 03:09:56 GMT+0800","2023-03-30T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Speed Log found showing incorrect values.","Navigation - Echo Sounder / Speed Log","Navigation","External Factors","","","","","Speed Log Sensor found shifted due to excessive pitching bu the vessel during rough weather. Same Re-positioned. Reading is satisfactory.","2023-06-29T23:59:35","NA","Completed","2023-04-03T23:59:35","No","No","No","Internal"]
[null,null,null,30707,57736,"0_Sun Apr 16 2023 01:57:52 GMT+0800","2023-04-01T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Wheelhouse Control Stand Microphone not operational.","Navigation - GMDSS & Communication","Navigation","Equipment Related","","","","","Mic renewed with new onboard spare. Tried out & in use.","2023-07-03T23:59:35","NA","Completed","2023-04-03T23:59:35","No","No","No","Internal"]
[null,null,null,30588,79244,"0_Sun Apr 16 2023 01:52:52 GMT+0800","2023-04-02T23:59:35","Observation","Ship Staff","Ship Staff Insp.","ME LO Autobackwash (Maotti) Filter Found with High Pressure Differential.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","1st Stage Filter Chamber found with lint/rags. Same Cleaned & boxed up. 2nd Stage Filter Chamber opened up for inspection. Found the filter mesh damaged. Renewed with spare filter elements. Vessel doesnot have nay spare filter set in case of emergency. RO DPUM230097 raised for same.  LO filter working normal now. As per suptd comments PO stands closed as of now. Will be supplied in emergency.","2023-07-02T23:59:35","RO DPUM230097","Completed","2023-08-20T23:59:35","No","No","No","Internal","ME LO Autobackwash (Maotti) Filter - High Pressure Differential - if returned back to normal, then the same is to be closed. RO DPUM230097 - for spare - in case required in future - will be supplied to the vessel at 1st opportunity."]
[null,null,null,30709,63686,"0_Sun Apr 16 2023 02:05:08 GMT+0800","2023-04-02T23:59:35","Observation","Ship Staff","Ship Staff Insp.","COT #2 P & S Tank Pressure Monitoring not showing correct value.","Inert Gas","Cargo / Ballast Systems","Equipment Related","","","","","Sensors renewed & calibration required. RO DPUM230095 raised for used spares.","2023-07-02T23:59:35","DPUM230095","Completed","2023-04-04T23:59:35","No","No","No","Internal"]
[null,null,null,30714,98731,"0_Sun Apr 16 2023 03:06:52 GMT+0800","2023-04-02T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Doctor Software not detecting the Doctor Unit.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","IT Support received & same carried out. Issue Resolved. Doctor Unit is online.","2023-07-02T23:59:35","NA","Completed","2023-04-23T23:59:35","No","No","No","Internal"]
[null,null,null,30708,28018,"53_Sun Apr 16 2023 02:01:11 GMT+0800","2023-04-04T23:59:35","Observation","Ship Staff","Ship Staff Insp.","AE #2 Turbocharger Turbine Nozzle Ring Screws, one allen screw has broken inside the casing.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Screw extracted. All Allen screws renewed with new onboard spares. Turbocharger boxed up & tried out. In order.","2023-07-04T23:59:35","NA","Completed","2023-04-05T23:59:35","No","No","No","Internal"]
[null,null,null,30710,85149,"53_Sun Apr 16 2023 02:48:39 GMT+0800","2023-04-05T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Steerigng Gear Sound Powered phone Headset mic not working.","Navigation - GMDSS & Communication","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Headset renewed with new onboard spare.","2023-07-05T23:59:35","NA","Completed","2023-04-06T23:59:35","No","No","No","Internal"]
[null,null,null,30711,63733,"53_Sun Apr 16 2023 02:56:23 GMT+0800","2023-04-07T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Main 16K Steam Dump Valve found sluggish during operation.","E/R - Boiler,Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Dump Controller opened up & found with excessive oil inside. Same cleaned & overhauled. Tried out & found in order.","2023-07-07T23:59:35","NA","Completed","2023-04-07T23:59:35","No","No","No","Internal"]
[null,null,null,30740,95746,"0_Sun Apr 16 2023 03:02:27 GMT+0800","2023-04-10T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Control Air Drier performance not satisfactory. Oil carry over in the Control Air","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Control Air Drier to be renewed with onboard new spare. Piping modification completed. Dryer installed & connected. The dryer was commissioned as per office instructions. Performance is satisfactory. No oil/water carryover in the control air system. Awaiting maker manual to assist in spare ordering & troubleshooting in the future.","2023-07-10T23:59:35","NA","Completed","2023-05-28T23:59:35","No","No","No","Internal"]
[null,null,null,30724,51376,"53_Sun Apr 30 2023 20:20:09 GMT+0800","2023-04-14T23:59:35","Observation","Ship Staff","Ship Staff Insp.","ME Unit #1 & #2 Drain Lines & Elbows found choked. This led to both units underpiston spaces having considerable qty of sludge/deposits.","E/R - Main Engine,E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Inappropriate Procedure","10.32","Very High","","","Elbows removed & manually cleared. Staff remined to Steam blow the drian line effectively.","2023-07-14T23:59:35","NA","Completed","2023-04-15T23:59:35","No","No","No","Internal","NA"]
[null,null,null,30723,60713,"53_Sun Apr 30 2023 20:35:30 GMT+0800","2023-04-15T23:59:35","Observation","Ship Staff","Ship Staff Insp.","ME Scavenge Drain Line found choked.","E/R - Main Engine,E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Inappropriate Procedure","10.32","Very High","","","Entire pipe sections removed & manually cleared. Incorrect procedure for Steam blowing the line. ER staff breifed on the correct procedure.","2023-07-15T23:59:35","NA","Completed","2023-04-18T23:59:35","No","No","No","Internal","NA"]
[null,null,null,30716,45973,"0_Sun Apr 30 2023 20:48:41 GMT+0800","2023-04-16T23:59:35","Observation","Ship Staff","Ship Staff Insp.","ER Vent Fan #1 found tripping on high current.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Blower swung out & checked. Found the One phase lug broken in the JUnction Box of the Motor. Same renewed with new spare. Blower tried out & in use.","2023-07-16T23:59:35","NA","Completed","2023-04-17T23:59:35","No","No","No","Internal","NA"]
[null,null,null,30717,39080,"0_Sun Apr 30 2023 20:51:39 GMT+0800","2023-04-17T23:59:35","Observation","Ship Staff","Ship Staff Insp.","ME LO Cooler 3-Way Valve leaking from the Valve shaft.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Shaft seal renewed. Tried out & in use.","2023-07-17T23:59:35","NA","Completed","2023-04-20T23:59:35","No","No","No","Internal","NA"]
[null,null,null,30718,54962,"0_Sun Apr 30 2023 20:55:18 GMT+0800","2023-04-18T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Hose Handling Crane (Port) Slewing Motor Oil Seal Pot found severely corroded & damaged","Deck - Machinery","Cargo / Ballast Systems","Equipment Related","","","","","Same fabricated & repaired in ER Workshop. Re-installed & tried out. In use.","2023-07-18T23:59:35","NA","Completed","2023-04-19T23:59:35","No","No","No","Internal","NA"]
[null,null,null,30719,46978,"0_Sun Apr 30 2023 21:00:12 GMT+0800","2023-04-20T23:59:35","Observation","Ship Staff","Ship Staff Insp.","ME Hydraulic Top Bracing #2 found oil leaking from the cylinder.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Unit #2 overhauled. All o-rings & gaskets renewed. Installed & in use.","2023-07-22T23:59:35","NA","Completed","2023-04-23T23:59:35","No","No","No","Internal","NA"]
[null,null,null,30720,28231,"0_Sun Apr 30 2023 21:03:49 GMT+0800","2023-04-21T23:59:35","Observation","Ship Staff","Ship Staff Insp.","EGCS Scrubber SW Inlet Pipeline after the Quenching Valve found leaking.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Leak was found from the weld seam. Both flange ends weld seams have been repaired as a precaution. Installed back. System tried out & found satisafactory.\n","2023-07-21T23:59:35","NA","Completed","2023-04-22T23:59:35","No","No","No","Internal","NA"]
[null,null,null,30725,10049,"53_Sun Apr 30 2023 21:16:53 GMT+0800","2023-04-21T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Mooring winch #7 Brake Securing Plates broke during Arrival Operations.","Deck - Mooring Machinery","Mooring","Equipment Related","9.14","Medium","","","Same renewed with vessel fabricated spare. Tried out & in order.","2023-07-21T23:59:35","NA","Completed","2023-04-21T23:59:35","No","No","No","Internal","NA"]
[null,null,null,30721,65528,"0_Sun Apr 30 2023 21:08:38 GMT+0800","2023-04-22T23:59:35","Observation","Ship Staff","Ship Staff Insp.","ME Unit #4, #5 & #6 Exhaust Valve Actuator Plug Screw leaking.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Same renewed with new onboard spares. Tried out & no leaks observed. RO to be raised for spares.","2023-07-22T23:59:35","","Completed","2023-04-23T23:59:35","No","No","No","Internal","NA"]
[null,null,null,30728,95559,"53_Mon May 15 2023 19:09:47 GMT+0800","2023-04-28T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Steering Gear #1 & #2 Cooling Fan Panel LED Lights found fused.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Same renewed with onboard new spares. Tried out & in order.","2023-07-29T23:59:35","NA","Completed","2023-04-30T23:59:35","No","No","No","Internal"]
[null,null,null,30737,53552,"0_Mon May 15 2023 19:21:37 GMT+0800","2023-04-28T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Aux Boiler #1 Port & Stbd Gauge glasses and Aux. Boiler #2 Stbd Gauge Glass found discloured.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Same overhauled. New gaskets & glass installed.  Boiler tried out & in order.","2023-07-29T23:59:35","NA","Completed","2023-05-04T23:59:35","No","No","No","Internal"]
[null,null,null,30729,65817,"0_Mon May 15 2023 19:16:43 GMT+0800","2023-04-29T23:59:35","Observation","Ship Staff","Ship Staff Insp.","AE FO Booster Pump #1 Motor found with slight abnormal noise.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Same opened up for inpection. Found Free end bearing slightly worn out. same renewed with new spare bearings. Motor tried out & found in order.","2023-07-30T23:59:35","NA","Completed","2023-05-01T23:59:35","No","No","No","Internal"]
[null,null,null,30731,10769,"0_Mon May 15 2023 19:23:52 GMT+0800","2023-04-29T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Aux. Cooling SW Pump found leaking from the mechanical seal.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Pump overhualed. Mechanical Seal renewed. SHaft & Wera rings in satisfactory condition. Same boxed back, installed & tried out. In order.","2023-07-30T23:59:35","NA","Completed","2023-05-05T23:59:35","No","No","No","Internal"]
[null,null,null,30730,39843,"0_Mon May 15 2023 19:19:19 GMT+0800","2023-04-30T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Deck Seal Pump #1 found leaking","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Mechanical Seal renewed with new onboard spare along. Pump also overhauled. Found wear rings in good condition. Shaft sleeve renewed with new spare. Pump installed back, tried out & in use.","2023-07-29T23:59:35","NA","Completed","2023-05-03T23:59:35","No","No","No","Internal"]
[null,null,null,30733,51381,"0_Mon May 15 2023 19:14:35 GMT+0800","2023-04-30T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Emcy Fire Pump Water found overflowing from priming chamber during starting.","Critical Equip.","Eng. / Strg. Comp.","Equipment Related","5.41","Very High","","","Primimg unit Check valve found getting stuck & not moving freely. Same overhauled/cleaned. Installed back & tried out. Emcy Fire pump in order.","2023-07-31T23:59:35","NA","Completed","2023-05-01T23:59:35","No","No","No","Internal"]
[null,null,null,30732,29366,"0_Mon May 15 2023 19:50:23 GMT+0800","2023-05-08T23:59:35","Observation","Ship Staff","Ship Staff Insp.","EGCS CEMS Unit CO2 reading showing 1.4~1.8 vol%","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Found the 3-way Solenoid valve (S0V00402) not holding & drawing air from the atmosphere. Same renewed with new spare. System tried out & running satisfactorily. RO \"DPUM230118\" raised for consumed spare.\n","2023-08-08T23:59:35","DPUM230118","Completed","2023-05-08T23:59:35","No","No","No","Internal"]
[null,null,null,30736,33219,"0_Mon May 15 2023 19:55:06 GMT+0800","2023-05-08T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Fwd Hydraulics SW Cooler Inlet Pipe found with pinhole leak.","Deck - Mooring Machinery,Deck - Pipe / Fittings","Mooring","Equipment Related","9.14","Medium","","","PIpe removed & brought to ER Workshop. Fabricated & renewed the complete pipe section. Same installed & tried out. In order.","2023-08-08T23:59:35","NA","Completed","2023-05-10T23:59:35","No","No","No","Internal"]
[null,null,null,30741,12309,"53_Mon May 15 2023 22:55:07 GMT+0800","2023-05-08T23:59:35","Observation","Ship Staff","Ship Staff Insp.","IG main line pressure gauge inside pump-room is nonoperational (not working)","Inert Gas","Cargo / Ballast Systems","External Factors","8.25","Very High","","","New pressure gauge received at Singapore was installed & found working satisfactory ","2023-06-27T23:59:35","DPUM230116-Stores","Completed","2023-05-29T23:59:35","No","No","No","Internal"]
[null,null,null,30738,99299,"0_Mon May 15 2023 20:04:14 GMT+0800","2023-05-09T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Electrical Insulation Gloves near Emcy Switrchboard found damaged.","Elect. Mach. & Equip.","Safety / LSA / FFA","Equipment Related","10.24","Low","","","RO \"DPUM230116\" raised for new spare. Received & replaced at all locations as certificate was due for expiration.","2023-08-09T23:59:35","DPUM230116","Completed","2023-05-29T23:59:35","No","No","No","Internal"]
[null,null,null,30747,75264,"53_Sun Jun 04 2023 15:45:38 GMT+0800","2023-05-12T23:59:35","Observation","Ship Staff","Ship Staff Insp.","OWS 1st Chamber Vent Valve leaking during operation","Critical Equip.","MARPOL Related","Equipment Related","10.32","Very High","","","Vent valve replaced with new onboard spare. System tried out. No leaks observed.","2023-08-14T23:59:35","NA","Completed","2023-05-14T23:59:35","No","No","No","Internal"]
[null,null,null,30599,12239,"53_Fri Jun 02 2023 19:48:21 GMT+0800","2023-05-12T23:59:35","Observation","Ship Staff","Ship Staff Insp.","During routine inspection & testing of sprinklers for chemical locker it has been found that one of the sprinkler nozzle head is deformed.","LSA / FFA","Safety / LSA / FFA","External Factors","5.35","Medium","","","Nozzle was removed & inspected.  RO for same has been raised.(PO number - DPUM 230130 ) Sprinkler received fitted in place. ","2023-06-27T23:59:35","DPUM 230130 (LSA/FFA STORE @ SINGAPORE)","Completed","2023-06-29T23:59:35","No","No","No","Internal","As the vessel has completed the fabrication of the nozzle on board, same can be closed in DDRL. DPUM 230130 - will be supplied at first opportunity."]
[null,null,null,30748,96854,"53_Sun Jun 04 2023 15:52:04 GMT+0800","2023-05-13T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Pump room High & Low Vent Suction Control Valve Cabinet damaged due to corrosion.","Critical Equip.","Emgcy. Systems","Equipment Related","5.18","High","","","Cabinet removed & replaced with onboard fabricated one. Installed & system tried out. In order.","2023-08-13T23:59:35","NA","Completed","2023-05-25T23:59:35","No","No","No","Internal"]
[null,null,null,30755,85082,"0_Sun Jun 04 2023 16:04:30 GMT+0800","2023-05-13T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Vent Head Covers found corroded & holed for Bunker Tank #1P & #1S","Deck - Pipe / Fittings","MARPOL Related","Equipment Related","11.7","High","","","Same removed & repaired by renewal of the material in the ER workshop. installed & in use.","2023-05-17T23:59:35","NA","Completed","2023-05-26T23:59:35","No","No","No","Internal"]
[null,null,null,30601,17789,"53_Mon Jun 05 2023 09:18:14 GMT+0800","2023-05-13T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Annual service of ODME Over DUE 15.05.2023","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","6.13","Low","","","ODME Annual shore service carried out on 28-June-2023 at Singapore.","2023-07-12T23:59:35","DPUM230122","Completed","2023-06-27T23:59:35","No","No","No","Internal",""]
[null,null,null,30749,49431,"0_Sun Jun 04 2023 15:57:22 GMT+0800","2023-05-14T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Mast riser Vent Cover Plate Damaged due to corrosion.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.19","High","","","Plate removed & renewed with onboard fabricated one. Same installed & in use.","2023-08-14T23:59:35","NA","Completed","2023-05-17T23:59:35","No","No","No","Internal"]
[null,null,null,30750,87474,"0_Sun Jun 04 2023 16:00:39 GMT+0800","2023-05-15T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Hose Handling Crane (Port) Man riding Hoisting limit switch not operating.","Deck - Machinery,Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.50","Medium","","","Limit switch adjusted. Tried out & in order.","2023-08-15T23:59:35","NA","Completed","2023-05-15T23:59:35","No","No","No","Internal"]
[null,null,null,30752,69580,"0_Sun Jun 04 2023 16:12:44 GMT+0800","2023-05-15T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Hose handling Crane (Stbd) Oil Seal pot found damaged/holed due to corrosion.","Cargo Mach.,Deck - Machinery","Cargo / Ballast Systems","Equipment Related","8.50","Medium","","","Same removed from place & repaired by welding in the ER Workshop. Installed back & crane tried out. In order.","2023-08-15T23:59:35","NA","Completed","2023-05-24T23:59:35","No","No","No","Internal"]
[null,null,null,30751,58432,"53_Sun Jun 04 2023 16:08:11 GMT+0800","2023-05-22T23:59:35","Observation","Ship Staff","Ship Staff Insp.","HFO Bunker Line Section found in slightly deteriorated condition due to corrosion.","Deck - Pipe / Fittings","General Appearance","Equipment Related","","","","","Section removed & renewed in ER Workshop. Installed back & line pressure tested up to 4.5bar. No leaks observed.","2023-08-22T23:59:35","NA","Completed","2023-05-25T23:59:35","No","No","No","Internal"]
[null,null,null,30600,46460,"53_Mon Jun 05 2023 09:14:31 GMT+0800","2023-05-22T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Various supports of fire line on sunken deck wasted heavily. Temporary repairs of same in progress . as they are IWO of bunker tanks HOT work can not be done","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","Equipment Related","11.4","Very High","","","Various supports of fire line on sunken deck repair completed.","2023-08-28T23:59:35","","Completed","2023-07-09T23:59:35","No","No","No","Internal",""]
[null,null,null,30602,75320,"53_Mon Jun 05 2023 09:21:56 GMT+0800","2023-05-22T23:59:35","Critical Equipment","Ship Staff","Ship Staff Insp.","Annual service of both Gyros over due 15.05.2023","Navigation - Others","Navigation","Equipment Related","4.9","Medium","","","Annual shore service of both Gyro compass carried out at Singapore on 28-June-2023.","2023-07-12T23:59:35","DPUM230087","Completed","2023-06-27T23:59:35","No","No","No","Internal",""]
[null,null,null,30753,42878,"0_Sun Jun 04 2023 16:17:51 GMT+0800","2023-05-26T23:59:35","Observation","Ship Staff","Ship Staff Insp.","AE #3 HT Temp trip while transferring onto full load","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Air Cooler leakage resulted in water carryover in the scavenge manifold. AE #3 Cylinder heads overhauled & found Liner top ring damaged for Unit #1, 2 & #3. All unit cylinder heads O-rings & gaskets renewed with new onboard spares. tried out & in order. Air Cooler End cover gasket renewed.  Cover gasket seating face damaged due to erosion. old cover replaced. tried out & in order. New end cover to be supplied.","2023-08-26T23:59:35","NA","Completed","2023-05-30T23:59:35","No","No","No","Internal"]
[null,null,null,30754,84600,"0_Wed Jun 14 2023 09:04:31 GMT+0800","2023-06-04T23:59:35","Observation","Ship Staff","Ship Staff Insp.","AE #1 Unit #4 Water leak from Telltale hole during starting.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Air Cooler End cover gasket leak. Same renewed with new spare. Unit #4 Cyl Head removed & LIner top o-ring found damaged. Same renewed with new spare. Old Cyl Head reused. AE Tried out & in order.","2023-09-04T23:59:35","NA","Completed","2023-06-04T23:59:35","No","No","No","Internal"]
[null,null,null,30604,53304,"53_Wed Jun 14 2023 09:00:54 GMT+0800","2023-06-04T23:59:35","Observation","Ship Staff","Ship Staff Insp.","WMS-002 Sampling Pump Low FLow Alarm & WMP-002 Pump Stop","E/R - Main Engine,E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Pump found unable to build pressure. Same renewed under GC-008-23 by Shore Technician at Ulsan on 13-Jun-2023. System to be tried out.System found running in good order","2023-09-04T23:59:35","GC-008-23","Completed","2023-07-30T23:59:35","No","No","No","Internal","Noted that the Pump renewed under GC-008-23 by Shore Technician at Ulsan on 13-Jun-2023. Do check if the pump performance is satisfactory, then this GC is to be closed."]
[null,null,null,31266,68555,"0_Sun Aug 20 2023 23:39:52 GMT+0800","2023-06-27T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Some vent flaps around external accommodation corroded.","Accommodation","Structural Condn. / WT integrity ","External Factors","11.8","Low","","","Derusting , painting  & maintenance of all Vent flaps around external accommodation completed. ","2023-08-11T23:59:35","","Completed","2023-07-28T23:59:35","No","No","No","Internal"]
[null,null,null,31267,25895,"0_Sun Aug 20 2023 23:41:22 GMT+0800","2023-06-27T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Port and Stbd bridge wing support pillar inboard section having rust.","Accommodation","General Appearance","External Factors","11.8","Low","","","Derusting , Buffing & Painting carried out.","2023-08-11T23:59:35","","Completed","2023-08-01T23:59:35","No","No","No","Internal"]
[null,null,null,31268,45224,"0_Sun Aug 20 2023 23:43:14 GMT+0800","2023-06-27T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","IG Line from Engine room block to main deck having rust near flanges.","Inert Gas,Deck - Pipe / Fittings","General Appearance","External Factors","11.4","Very High","","","Derusting,Buffing & painting carried out.","2023-08-11T23:59:35","","Completed","2023-07-27T23:59:35","No","No","No","Internal"]
[null,null,null,31269,82991,"0_Sun Aug 20 2023 23:47:24 GMT+0800","2023-06-27T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Brake band of all mooring winches rusted and require maintenance.","Deck - Mooring Machinery","Mooring","External Factors","9.14","Medium","","","Derusting , Painting & renewal of brake pads for aft mooring winches completed.","2023-08-26T23:59:35","","Completed","2023-07-30T23:59:35","No","No","No","Internal"]
[null,null,null,31270,54147,"0_Sun Aug 20 2023 23:46:03 GMT+0800","2023-06-27T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Midship crane having rust stains.","Deck - Machinery","General Appearance","External Factors","11.3","Medium","","","Derusting , Buffing & Painting carried out.","2023-08-26T23:59:35","","Completed","2023-07-31T23:59:35","No","No","No","Internal"]
[null,null,null,31271,28929,"53_Sun Aug 20 2023 23:37:45 GMT+0800","2023-06-27T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Some cable penetration for the external accommodation light corroded with rust stains.","Elect. Mach. & Equip.,Accommodation","General Appearance","External Factors","11.10","Medium","","","Derusting , Buffing & Painting completed.","2023-08-11T23:59:35","","Completed","2023-08-03T23:59:35","No","No","No","Internal"]
[null,null,null,31272,10779,"0_Sun Aug 20 2023 23:53:29 GMT+0800","2023-06-27T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Deck below pipelines from manifold to forecastle decolorized by rust stains.","Miscellaneous","General Appearance","External Factors","11.3","Medium","","","Deck below pipelines from manifold to forecastle rust stain marks cleaned. Few spots re-panted.","2023-08-30T23:59:35","","Completed","2023-08-21T23:59:35","No","No","No","Internal","Extension granted as per mail request from vessel for same till 31-Aug-2023."]
[null,null,null,31273,10592,"0_Sun Aug 20 2023 23:50:29 GMT+0800","2023-06-27T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Cable supports from manifold to forecastle found to be corroded.","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","External Factors","11.5","Medium","","","Cable supports from manifold to forecastle derusting & painting  completed.","2023-08-26T23:59:35","","Completed","2023-08-17T23:59:35","No","No","No","Internal"]
[null,null,null,31274,37030,"0_Sun Aug 20 2023 23:44:14 GMT+0800","2023-06-27T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","3W COW Line root valve and machine valve rusted.","Deck - Pipe / Fittings","Cargo / Ballast Systems","External Factors","11.5","Medium","","","3W COW Line root valve and machine valve derusting & painting completed. Marking also done.","2023-08-14T23:59:35","","Completed",null,"No","No","No","Internal"]
[null,null,null,null,36975,"0_Sun Aug 20 2023 23:54:40 GMT+0800","2023-06-27T08:00:00","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","IG Pipeline flanges from manifold to forecastle corroded.","Deck - Pipe / Fittings,Inert Gas","Cargo / Ballast Systems","External Factors","11.5","Medium","","","IG Pipeline flanges from manifold to forecastle Spot derusting and painting for main deck lines & fitting carried out.","2023-08-30T08:00:00","","Completed","2023-08-25T08:00:00","No","No","No","Internal"]
[null,null,null,null,82100,"0_Sun Aug 20 2023 23:51:31 GMT+0800","2023-06-27T08:00:00","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Mast riser valve and Breather valve corroded.","Inert Gas,Deck - Pipe / Fittings","Cargo / Ballast Systems","External Factors","11.5","Medium","","","Mast riser valve and Breather valve de-rusting and painting carried out.","2023-08-30T08:00:00","","Completed","2023-08-25T08:00:00","No","No","No","Internal","Extension granted as per request mail from vessel for same till 31-aug-2023."]
[null,null,null,null,82735,"0_Sun Aug 20 2023 23:49:05 GMT+0800","2023-06-27T08:00:00","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Foam monitor platform and ladder rusted.","LSA / FFA","Structural Condn. / WT integrity ","External Factors","11.3","Medium","","","Foam monitor platform and ladder de-rusting/painting completed. Cosmetic up gradation completed.","2023-08-30T08:00:00","","Completed","2023-08-25T08:00:00","No","No","No","Internal","Extension granted as per email request from vessel for same till 31-aug-2023."]
[null,null,null,null,27062,"53_Thu Sep 14 2023 19:46:09 GMT+0800","2023-08-29T08:00:00","Other","Ship Staff","Ship Staff Insp.","Vessel inspected Water Ballast Tank, found indentation in 1P, 2P and 3P Water Ballast tanks at various location as following:\nAA. Indentation in 1P water Ballast Tank\n1)At 1st Stringer between Frame No. 99 & 100, close to Frame 99, indentation of following measurement, \nDepth : 15 cms; Width : 1 mtr ; Length : 4.1 mtr on Horizontal girder No-53 \n2) Between frame No.100 & 101, Close to Frame no.100, indentation of following measurement, \nDepth : 7 cm; Width : 550 cms; Length : 1.2 Mts; on side longitudinal No-54\n3) Ship side shell plating between longitudinal 53 to 54 and in between frame 99-100 has a indentation of about ½ to 1 Cm,\n4) Ship side shell plating between longitudinal 53 to 54 and in between frame 97-98 also has a small indentation of about ½.\n5) Paint abrasion is seen at some places between frame 98-100 and longitudinal 53-54. \n\nBB. Indentation in 2P water Ballast Tank\n1)\tAt 1st Stringer between Frame No. 90 & 91, Close to Frame 90, Indentation of following measurement, \nDepth : 5 cms; Width : 0.8 mtr ; Length : 1.2 mtr, between horizontal longitudinal 54-55 (sea side)\n  2)\tAt 1st Stringer between Frame No. 90 & 91, Close to Frame 90, Indentation of following measurement, \nDepth : 5 cms; Width : 0.8 mtr ; Length : 1.2 mtr, between horizontal longitudinal 53-54 (sea side) \n3)\tAt 1st Stringer between Frame No. 89 & 90, Close to Frame 90, Indentation of following measurement, \nDepth : 3 cms; Width : 1.0 mtr ; Length : 2.0 mtr, between horizontal longitudinal 54-55 (sea side)\n\nCC. Indentation in 3P water Ballast Tank\n1)\tAt 3rd Stringer between Frame No. 81 & 82, Close to Frame 81, Indentation of following measurement, \nDepth: 4cms; Width: 0.20mtr; Length: 0.40mts, near horizontal longitudinal 38 (sea side)\n\n","Hull & Tanks","Cargo / Ballast Systems","External Factors","2.9","Medium","","","Vessel raised dry dock repair for indentation in ballast tank in REFMAN. Deck Jobs No. DK-10, DK-11 & DK-12","2023-11-14T08:00:00","","Completed","2023-09-14T08:00:00","No","No","No","Internal"]
[null,null,null,null,91945,"0_Wed Feb 22 2023 17:45:13 GMT+0800","2023-02-12T08:00:00","Observation","Ship Staff","Ship Staff Insp.","Kyma computer monitor display is blurred.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","The display monitor was replaced with new but still the problem exists.\nKindly check with maker - if it is software/ setting issue . target date revised .\nVGA cable Renewed and problem solved.","2023-10-30T08:00:00","","Completed","2023-08-21T08:00:00","No","No","No","Internal","Please advise the plan for corrective action."]
[null,null,null,null,11843,"0_Wed Feb 22 2023 17:41:13 GMT+0800","2023-02-12T08:00:00","Observation","Ship Staff","Ship Staff Insp.","Some hydraulic pipelines on deck for remote winch operation need replacement.","Deck - Pipe / Fittings","Mooring","Equipment Related","11.4","Very High","","","PIpe sections to be removed & repaired in the ER Workshop. 01.05.2023 also remote operating levers to be tested. One winch completed one more will be planned shortly. Have chipped and found second suspected winch remote operation pipe in good condition and does not require renewal.","2023-10-30T08:00:00","NA","Completed","2023-09-09T08:00:00","No","No","No","Internal","Please advise progress"]
[null,null,null,null,45220,"53_Wed Jun 14 2023 09:13:25 GMT+0800","2023-06-09T08:00:00","Observation","Ship Staff","Ship Staff Insp.","Fwd Hydraulic Starter Panel PLC defective.","Deck - Machinery","Eng. / Strg. Comp.","Equipment Related","9.20","Medium","","","Vessel renewed with new PLC received in Singapore.\nChecked the system and found operation good. \nJob plan : V-DPUM049524/23 reported in PMS.","2023-10-30T08:00:00","DPUM230042","Completed","2023-10-23T08:00:00","No","No","No","Internal","DPUM230042 - noted on the PO raised for Fwd Hydraulic Starter Panel PLC defective. Once received, install the same and advise."]
[null,null,null,null,14624,"53_Sun Apr 30 2023 20:44:58 GMT+0800","2023-04-15T08:00:00","Observation","Ship Staff","Ship Staff Insp.","FW Tank (Port) Level Gauge faulty.","Hull & Tanks","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Spare gauge received in Singapore. \nsame fitted and Gauge working. \nJo plan:  V-DPUM049525/23 reported in PMS.\n\n","2023-10-30T08:00:00","DPUM230106","Completed","2023-10-21T08:00:00","No","No","No","Internal","RO \"DPUM230106\" - will be supplied to the vessel at Singapore in June 2023."]
[null,null,null,null,38828,"53_Fri Sep 15 2023 09:53:52 GMT+0800","2023-09-11T08:00:00","Observation","Ship Staff","Ship Staff Insp.","Vessel found one DCP semi portable fire extinguisher 25 kg (Pressure type) pressure gauge indicator slighlty higher than normal range (in red zone)  located in mid-ship store.","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.42","Medium","","","Vessel received new DCP semi portable fire extinguisher 25 KG at Singapore on 17-Oct-2023. Vessel replaced defective extinguisher.","2023-10-30T08:00:00","","Completed","2023-10-17T08:00:00","No","No","No","Internal"]
[null,null,null,null,66828,"53_Thu Sep 14 2023 19:33:25 GMT+0800","2023-09-08T08:00:00","Observation","Ship Staff","Ship Staff Insp.","FPK Water Ballast tank vent heads (Air pipes) 3 Nos Size 65A,  body wasted and rusted, required renewal.","Deck - Pipe / Fittings","Cargo / Ballast Systems","External Factors","11.7","High","","","Vessel received 3 sets of Ballast tank vent heads (Size: 65A)  at Singapore on 17-Oct-2023. Vessel replaced damage vent heads with new one. Painting and marking carried out.","2023-10-31T08:00:00","DPUM230187: BALLAST TANK VENT (AIR PIPE)","Completed","2023-10-24T08:00:00","No","No","No","Internal"]
[null,null,null,null,64752,"0_Thu Feb 23 2023 17:58:24 GMT+0800","2023-02-12T08:00:00","Observation","Ship Staff","Ship Staff Insp.","APT BWTS end plates are bipolar plates to be renewed.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","6.21","High","","","26 Plates received and same renewed. Total is 40 hence 14 old plates used.\nSystem tried out.","2023-10-30T08:00:00","DPUM230021","Completed","2023-10-07T08:00:00","No","No","No","Internal","Noted on End Plate RO DPUM230021.\n\nHow many Bi Polar plates vessel is having as spare?"]
[null,null,null,null,43975,"53_Mon May 15 2023 21:03:14 GMT+0800","2023-04-21T08:00:00","Observation","Ship Staff","Ship Staff Insp.","ME Fuel Valve Testing Device found leaking oil.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Spares received and renewed. All in order.","2023-10-30T08:00:00","Quotation No.: S2220768536","Completed","2023-09-25T08:00:00","No","No","No","Internal","Quotation No.: S2220768536 - should have be supplied to the vessel at Singapore in June 2023."]
[null,null,null,null,20393,"0_Mon May 15 2023 20:46:58 GMT+0800","2023-05-03T08:00:00","Observation","Ship Staff","Ship Staff Insp.","ME Unit #2 & #3 Exhaust Valve Actuator Plug screws leaking.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Vessel ROB of spare plug screws is NIL. Unit #2 renewed at Port Louis on 19-May-2023. Spares Received under RO \"DPUM230109\".  Renewed for # 3 Unit.","2023-11-15T08:00:00","DPUM230109","Completed","2023-10-30T08:00:00","No","No","No","Internal","Noted that #3 Exhaust Valve Actuator Plug screws leaking. RO \"DPUM230109\" to be supplied to the vessel at first Opportunity."]
[null,null,null,null,10669,"53_Fri Nov 03 2023 14:42:54 GMT+0800","2023-10-30T08:00:00","Defect","Ship Staff","Ship Staff Insp.","AE #2 Pickup Sensor for Doctor Unit malfunctioning.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Vessel has checked all the connections, and the pickup was cleaned. The pickup was  tested multiple times, and is found in good working order.","2023-12-15T08:00:00","","Completed","2023-11-10T08:00:00","No","No","No","Internal"]
[null,null,null,null,49753,"0_Mon May 15 2023 20:44:05 GMT+0800","2023-05-08T08:00:00","Observation","Ship Staff","Ship Staff Insp.","Flourscent light terminal box fittings in engine room were observed with damage.","Elect. Mach. & Equip.","General Appearance","Equipment Related","11.10","Medium","","","Received Spares and changed as required.","2023-12-15T08:00:00","","Completed","2023-11-10T08:00:00","No","No","No","Internal","Noted that received wring dimension terminal boxes under DPUM235018 - which was not correct. Correct type - terminal boxes has been ordered to Anhai in China in June 2023."]
[null,null,null,null,24951,"53_Fri Nov 03 2023 21:48:46 GMT+0800","2023-11-02T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Wind direction cup of anemometer was found broken. \nIsolation transformer found burnt.","Navigation - Others","Navigation","Equipment Related","4.7","High","","","RO raised for Wind direction cup . DPUM230235\n\nTransformer sourced temporarily and RO raised for Isolation Transformer . DPUM230230\nnew anemometer received. Same has been mounted in place and working for past 3 days. This job being closed now.","2023-12-15T08:00:00","","Completed","2023-12-12T08:00:00","No","No","No","Internal"]
[null,null,null,null,28903,"53_Fri Dec 15 2023 18:41:49 GMT+0800","2023-12-07T08:00:00","Breakdown","Ship Staff","Ship Staff Insp.","Midship crane STBD return filter body found crack.","Deck - Machinery","Cargo / Ballast Systems","Equipment Related","8.50","Medium","","","New spare received under DPUM235109 including the filter along with body and same replaced. Found size of the filter is small compared to the removed one and same have been notified to office.","2023-12-15T08:00:00","","Completed","2023-12-11T08:00:00","No","No","No","Internal"]
[null,null,null,null,36291,"53_Fri Dec 15 2023 18:46:36 GMT+0800","2023-12-02T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Hydroblaster safety valve is leaking and not able to maintain pressure. ","Deck - Machinery","General Appearance","Equipment Related","","","","","Spares received for relief valve and same renewed and tried out. Found in order and working fine.","2023-12-15T08:00:00","","Completed","2023-12-15T08:00:00","No","No","No","Internal"]
[null,null,null,null,55199,"53_Sun Dec 17 2023 13:04:14 GMT+0800","2023-12-08T08:00:00","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","“Use Trailing Hand Technique” stencil missing on exterior ladders from Monkey Island upto B-Deck.","Accommodation","General Appearance","Human Error","11.1","High","","","Missing stencils on ladder marked with use trailing hand techniques.","2023-12-23T08:00:00","","Completed","2023-12-15T08:00:00","No","No","No","Internal"]
[null,null,null,null,63592,"53_Sun Dec 17 2023 13:13:15 GMT+0800","2023-12-08T08:00:00","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Fire Hose Box on C-Deck (Port Side) Support de-rusting and painting","LSA / FFA","General Appearance","External Factors","5.38","High","","","Deeusting and painting on Fire Hose Box port side on C Deck Completed.","2023-12-23T08:00:00","","Completed","2023-12-14T08:00:00","No","No","No","Internal"]
[null,null,null,null,96456,"53_Sun Dec 17 2023 13:39:12 GMT+0800","2023-12-08T08:00:00","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","C-Deck (Port Side) Light Supports (2 Nos) Soft patch to be repaired.","Miscellaneous","General Appearance","External Factors","11.1","High","","","C Deck portside light supports 2 nos soft patches removed, derusting and painting carried out.","2024-03-23T08:00:00","","Completed","2023-12-16T08:00:00","No","No","No","Internal"]
[null,null,null,null,96810,"53_Sun Dec 17 2023 13:42:59 GMT+0800","2023-12-08T08:00:00","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","AC Vent door Rubber packing to be renewed and Coaming derusting and painting.","Accommodation","General Appearance","External Factors","11.1","High","","","Ac vent door rubber packing renewed, complete duristing and painting of coaming carried out.","2024-03-23T08:00:00","","Completed","2023-12-16T08:00:00","No","No","No","Internal"]
[null,null,null,null,87111,"53_Sun Dec 17 2023 13:50:17 GMT+0800","2023-12-08T08:00:00","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","OPEN – SHUT Marking on Engine Room Blower.","Miscellaneous","General Appearance","External Factors","11.8","Low","","","Open shut markings on E/R blower were carried out.","2023-12-23T08:00:00","","Completed","2023-12-14T08:00:00","No","No","No","Internal"]
[null,null,null,null,13888,"53_Sun Dec 17 2023 14:15:38 GMT+0800","2023-12-08T08:00:00","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Securing Rope for both Provision Crane Hook and Fwd Bosun store davit to replace with less SWL.","Cargo Mach.","","Inappropriate Procedure","8.50","Medium","","","Both provision crane Hook and fwd Davit securing ropes renewed with lesser SWL.","2023-12-23T08:00:00","","Completed","2023-12-13T08:00:00","No","No","No","Internal"]
[null,null,null,null,26651,"53_Sun Dec 17 2023 14:19:23 GMT+0800","2023-12-08T08:00:00","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","1 no Accommodation porthole rubber packing dislodged (2nd Window from Port (Blower deck) – Aft)","Accommodation","Structural Condn. / WT integrity ","External Factors","11.6","Medium","","","Porthole dislodged rubber packing placed back in place and fixed.","2023-12-15T08:00:00","","Completed","2023-12-12T08:00:00","No","No","No","Internal"]
[null,null,null,null,22485,"53_Sun Dec 17 2023 14:25:52 GMT+0800","2023-12-08T08:00:00","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Embarkation light (P & S) on boat deck horizontal and vertical movement to be freed up.","LSA / FFA","Safety / LSA / FFA","External Factors","5.30","High","","","Port & Stbd embarkation lights on boat deck movment freed up and in order.","2023-12-15T08:00:00","","Completed","2023-12-12T08:00:00","No","No","No","Internal"]
[null,null,null,null,21335,"53_Sun Dec 17 2023 22:24:00 GMT+0800","2023-12-08T08:00:00","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Hydro blaster unable to maintain pressure.","Miscellaneous","General Appearance","Equipment Related","11.4","Very High","","","Hydroblaster unit repaired with spares received, damaged hoses changed and leaks rectified. Hydroblaster pressure maintaining 800 Bar  under obsaervation.","2024-03-23T08:00:00","","Completed","2023-12-15T08:00:00","No","No","No","Internal"]
[null,null,null,null,59130,"53_Sun Dec 17 2023 22:34:25 GMT+0800","2023-12-08T08:00:00","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Various stencils on deck are missing due to being freshly painted. Same to be re-stenciled.","Deck - Mooring Machinery","Mooring","Human Error","11.1","High","","","Various stencilling of Deck completed and in progress as required.","2024-01-08T08:00:00","","Completed","2023-12-16T08:00:00","No","No","No","Internal"]
[null,null,null,null,93478,"53_Sun Dec 17 2023 22:38:21 GMT+0800","2023-12-08T08:00:00","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Photographic procedures to be made for Emergency crane operation.","Cargo Mach.","General Appearance","Inappropriate Procedure","8.50","Medium","","","Photogrphic procedures for emergency crane operations made and kept ready.","2024-01-08T08:00:00","","Completed","2023-12-13T08:00:00","No","No","No","Internal"]
[null,null,null,null,56249,"53_Mon Dec 04 2023 10:33:03 GMT+0800","2023-11-27T08:00:00","Observation","Ship Staff","Ship Staff Insp.","BWTS for main ballast tank Rectifer unit A & C not operational. ","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","6.21","High","","","Shore technician at singapore on 08-Dec-23 attended the BWTS rectifier unit. System was tried out for twice anf all rectifiers are now in good working order.","2023-12-31T08:00:00","","Completed","2023-12-18T08:00:00","No","No","No","Internal"]
[null,null,null,null,25028,"53_Thu Feb 23 2023 17:51:06 GMT+0800","2023-02-12T08:00:00","Observation","Ship Staff","Ship Staff Insp.","Main BWTS both filters are back flushing continuously.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","6.21","High","","","At Singapore on 08-Dec-23, BWTS system NF upgrade was completed. Hence this is not applicable to the vessel any more.","2023-12-30T08:00:00","","Completed","2023-12-08T08:00:00","No","No","No","Internal","Please resend the email for our follow up."]

{"sheet":"Calc","index":2,"n_rows":28,"n_cols":12,"rows_kept":28,"cut":false,"hidden":true,"merged":[]}
["Def_type","Def_cause","Equipments","VIQrefno","Observer_code"]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,"Dim itemSele As Long"]
[null,null,null,null,null,null,null,null,null,null,null,"   dim startRow as integer"]
[null,null,null,null,null,null,null,null,null,null,null,"   startRow=1"]
[null,null,null,null,null,null,null,null,null,null,null,"        For itemSele = 0 To ListBox1.ListCount - 1"]
[null,null,null,null,null,null,null,null,null,null,null,"        If ListBox1.Selected(itemSele) = True Then"]
[null,null,null,null,null,null,null,null,null,null,null,"        Worksheets(\"WorksheetName\").Range(\"A\" & startRow).Value = ListBox1.List(itemSele)"]
[null,null,null,null,null,null,null,null,null,null,null,"        startRow = startRow + 1"]
[null,null,null,null,null,null,null,null,null,null,null,"        End If"]
[null,null,null,null,null,null,null,null,null,null,null,"        Next"]
[null,null,null,null,null,null,null,null,null,null,null,"Dim LastRowA As String"]
[null,null,null,null,null,null,null,null,null,null,null,"        Dim itemSele As Long"]
[null,null,null,null,null,null,null,null,null,null,null,"       Dim startRow as integer"]
[null,null,null,null,null,null,null,null,null,null,null,"        LastRowA = ActiveSheet.Cells(Rows.count, \"A\").End(xlUp).row"]
[null,null,null,null,null,null,null,null,null,null,null,"        startQue = 0"]
[null,null,null,null,null,null,null,null,null,null,null,"        For itemSele = 0 To ListBox1.ListCount - 1"]
[null,null,null,null,null,null,null,null,null,null,null,"        For startRow = 1 To LastRowA"]
[null,null,null,null,null,null,null,null,null,null,null,"        If Worksheets(\"WorksheetName\").Range(\"A\" & startRow).Value = ListBox1.List(itemSele) Then"]
[null,null,null,null,null,null,null,null,null,null,null,"        ListBox1.Selected(itemSele) = True"]
[null,null,null,null,null,null,null,null,null,null,null,"        Exit For"]
[null,null,null,null,null,null,null,null,null,null,null,"        End If"]
[null,null,null,null,null,null,null,null,null,null,null,"        Next j"]
[null,null,null,null,null,null,null,null,null,null,null,"        Next"]
[null,null,null,null,null,null,null,null,null,null,null,"        End If"]

{"sheet":"Areaofobs","index":3,"n_rows":17,"n_cols":2,"rows_kept":17,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Cargo / Ballast Systems",11]
["Cert. & Docu.",2]
["Communication",6]
["Crew Management",3]
["Emgcy. Systems",13]
["Eng. / Strg. Comp.",14]
["General Appearance",15]
["Ice Opns.",17]
["ISM Related",7]
["ISPS Related",10]
["MARPOL Related",9]
["MLC Related",4]
["Mooring",12]
["Navigation",5]
["Safety / LSA / FFA",8]
["Structural Condn. / WT integrity ",16]

{"sheet":"Vessel_type","index":4,"n_rows":1,"n_cols":2,"rows_kept":1,"cut":false,"hidden":true,"merged":[]}
["Vessel_type","ID"]

{"sheet":"Deficiency_type","index":5,"n_rows":8,"n_cols":3,"rows_kept":8,"cut":false,"hidden":true,"merged":[]}
["TITLE","Type of deficiency_description","ID"]
["Breakdown",null,6]
["Critical Equipment",null,4]
["Defect",null,1]
["Guarantee Claim",null,8]
["Non Conformity",null,2]
["Observation",null,3]
["Other",null,7]

{"sheet":"VIQrefno","index":6,"n_rows":427,"n_cols":3,"rows_kept":427,"cut":false,"hidden":true,"merged":[]}
["VIQ_ref_no","Risk Value of observation","ID"]
["1.1","Low",8243]
["1.10","Low",8252]
["1.11","Low",8253]
["1.12","Low",8254]
["1.13","Low",8255]
["1.14","Low",8256]
["1.15","Low",8257]
["1.16","Low",8259]
["1.17","Low",8260]
["1.18","Low",8261]
["1.19","Low",8262]
["1.2","Low",8244]
["1.20","Low",8263]
["1.21","Low",8265]
["1.22","Low",8266]
["1.23","Low",8267]
["1.24","Low",8268]
["1.25","Low",8269]
["1.26","Low",8270]
["1.3","Low",8245]
["1.4","Low",8246]
["1.5","Low",8247]
["1.6","Low",8248]
["1.7","Low",8249]
["1.8","Low",8250]
["1.9","Low",8251]
["1.99","High",11258]
["10.1","Medium",8461]
["10.10","High",8470]
["10.11","Medium",8471]
["10.12","Very High",8472]
["10.13","Very High",8473]
["10.14","Medium",8474]
["10.15","Low",8475]
["10.16","Very High",8476]
["10.17","Very High",8477]
["10.18","High",8478]
["10.19","Very High",8479]
["10.2","Low",8462]
["10.20","High",8480]
["10.21","Medium",8481]
["10.22","Low",8482]
["10.23","Medium",8483]
["10.24","Low",8484]
["10.25","Very High",8485]
["10.26","High",8486]
["10.27","Medium",8487]
["10.28","Low",8488]
["10.29","Medium",8489]
["10.3","Medium",8463]
["10.30","High",8490]
["10.31","Very High",8491]
["10.32","Very High",8492]
["10.33","High",8493]
["10.34","High",8494]
["10.35","Very High",8495]
["10.36","Very High",8496]
["10.37","Medium",8497]
["10.38","Medium",8498]
["10.39","High",8499]
["10.4","High",8464]
["10.40","Medium",8500]
["10.41","Medium",8501]
["10.42","Medium",8502]
["10.43","Medium",8503]
["10.44","Medium",8504]
["10.45","Very High",8505]
["10.46","High",8506]
["10.47","Medium",8507]
["10.48","High",8508]
["10.49","Medium",8509]
["10.5","Low",8465]
["10.50","High",8510]
["10.51","Low",8511]
["10.52","Medium",8512]
["10.53","Medium",8513]
["10.54","High",8514]
["10.55","Low",8515]
["10.6","Very High",8466]
["10.7","Medium",8467]
["10.8","Medium",8468]
["10.9","Medium",8469]
["10.99","High",8516]
["11.1","High",8420]
["11.10","Medium",8429]
["11.11","Very High",8430]
["11.12","Low",8431]
["11.13","Low",8432]
["11.14","Medium",8433]
["11.15","Low",8434]
["11.16","Low",8435]
["11.17","Low",8436]
["11.2","Medium",8421]
["11.3","Medium",8422]
["11.4","Very High",8423]
["11.5","Medium",8424]
["11.6","Medium",8425]
["11.7","High",8426]
["11.8","Low",8427]
["11.9","Low",8428]
["11.99","High",8437]
["12.1","High",8438]
["12.10","High",8448]
["12.11","High",8449]
["12.12","High",8450]
["12.13","High",8451]
["12.14","High",8452]
["12.15","High",8453]
["12.16","High",8454]
["12.17","High",8455]
["12.18","High",8456]
["12.19","High",8457]
["12.2","High",8439]
["12.20","High",8458]
["12.21","High",8459]
["12.3","High",8441]
["12.4","High",8442]
["12.5","High",8443]
["12.6","High",8444]
["12.7","High",8445]
["12.8","High",8446]
["12.9","High",8447]
["12.99","High",8460]
["2.1","Very High",8296]
["2.1.9","Very High",11259]
["2.10","Medium",8304]
["2.11","Medium",8305]
["2.12","Low",8306]
["2.13","Low",8307]
["2.14","Low",8308]
["2.15","Low",8309]
["2.16","Medium",8310]
["2.2","Medium",8297]
["2.3","High",8295]
["2.4","Medium",8298]
["2.5","Medium",8299]
["2.6","Low",8300]
["2.7","High",8301]
["2.8","High",8302]
["2.9","Medium",8303]
["2.99","High",8311]
["3.1","High",8312]
["3.2","Very High",8313]
["3.3","High",8314]
["3.4","Low",8294]
["3.5","Medium",8315]
["3.6","High",8316]
["3.7","Very High",8317]
["3.8","Very High",8318]
["3.99","High",8319]
["4.1","High",8320]
["4.10","High",8329]
["4.11","Medium",8330]
["4.12","Very High",8331]
["4.13","Very High",8332]
["4.14","Very High",8333]
["4.15","Very High",8334]
["4.16","Very High",8335]
["4.17","Very High",8336]
["4.18","Very High",8337]
["4.19","Low",8338]
["4.2","Medium",8321]
["4.20","Very High",8339]
["4.21","High",8340]
["4.22","Low",8341]
["4.23","High",8342]
["4.24","High",8343]
["4.25","Low",8344]
["4.26","Low",8345]
["4.27","High",8346]
["4.3","Medium",8322]
["4.4","High",8323]
["4.5","Very High",8324]
["4.6","Medium",8325]
["4.7","High",8326]
["4.8","Medium",8327]
["4.9","Medium",8328]
["4.99","High",8347]
["5.1","Very High",8517]
["5.10","High",8526]
["5.11","Low",8527]
["5.12","Medium",8528]
["5.13","High",8529]
["5.14","Very High",8530]
["5.15","Medium",8531]
["5.16","Very High",8532]
["5.17","Very High",8533]
["5.18","High",8534]
["5.19","Medium",8535]
["5.2","Very High",8518]
["5.20","Medium",8536]
["5.21","Medium",8537]
["5.22","High",8539]
["5.23","Very High",8540]
["5.24","Very High",8541]
["5.25","Medium",8542]
["5.26","Medium",8543]
["5.27","Medium",8544]
["5.28","Very High",8545]
["5.29","High",8546]
["5.3","Low",8519]
["5.30","High",8547]
["5.31","High",8548]
["5.32","High",8549]
["5.33","High",8550]
["5.34","Low",8551]
["5.35","Medium",8552]
["5.36","Low",8553]
["5.37","Low",8554]
["5.38","High",8555]
["5.39","Very High",8556]
["5.4","High",8520]
["5.40","Very High",8557]
["5.41","Very High",8558]
["5.42","Medium",8559]
["5.43","High",8560]
["5.44","High",8561]
["5.45","Medium",8564]
["5.46","Medium",8565]
["5.47","Medium",8566]
["5.48","Medium",8567]
["5.5","Low",8521]
["5.6","Low",8522]
["5.7","Medium",8523]
["5.8","Medium",8524]
["5.9","Very High",8525]
["5.99","High",8568]
["6.1","Medium",8348]
["6.10","Low",8357]
["6.11","High",8358]
["6.12","Medium",8359]
["6.13","Low",8360]
["6.14","High",8361]
["6.15","High",8362]
["6.16","Very High",8363]
["6.17","Very High",8364]
["6.18","Medium",8365]
["6.19","Low",8366]
["6.2","High",8349]
["6.20","Medium",8367]
["6.21","High",8368]
["6.22","Medium",8369]
["6.3","Low",8350]
["6.4","High",8351]
["6.5","Medium",8352]
["6.6","Medium",8353]
["6.7","High",8354]
["6.8","High",8355]
["6.9","Low",8356]
["6.99","High",8370]
["7.1","High",8371]
["7.10","High",8380]
["7.11","High",8381]
["7.12","High",8382]
["7.13","Medium",8383]
["7.14","Medium",8384]
["7.15","High",8385]
["7.16","High",8386]
["7.17","High",8387]
["7.2","High",8372]
["7.3","Low",8373]
["7.4","Low",8374]
["7.5","Low",8375]
["7.6","Medium",8376]
["7.7","Low",8377]
["7.8","High",8378]
["7.9","High",8379]
["7.99","High",8388]
["8.1","Very High",8569]
["8.10","Very High",8578]
["8.100","Low",11227]
["8.101","Medium",11228]
["8.102","Low",11229]
["8.103","Low",11230]
["8.104","Low",11231]
["8.105","Medium",11232]
["8.106","Medium",11233]
["8.107","Low",11234]
["8.108","High",11235]
["8.109","Very High",11236]
["8.11","Medium",8579]
["8.110","High",11237]
["8.111","Medium",11238]
["8.112","High",11239]
["8.113","Medium",11240]
["8.114","Low",11241]
["8.115","High",11242]
["8.116","Medium",11243]
["8.117","Medium",11244]
["8.118","Medium",11245]
["8.119","High",11246]
["8.12","Medium",8580]
["8.120","High",11247]
["8.121","Medium",11248]
["8.122","High",11249]
["8.123","High",11250]
["8.124","Low",11251]
["8.125","High",11252]
["8.126","Medium",11253]
["8.127","Medium",11254]
["8.13","Medium",8581]
["8.14","Very High",8582]
["8.15","High",8583]
["8.16","Very High",8584]
["8.17","Low",8585]
["8.18","High",8586]
["8.19","High",8587]
["8.199","High",11255]
["8.2","Medium",8570]
["8.20","Medium",8588]
["8.21","High",8589]
["8.22","Very High",8590]
["8.23","Medium",8591]
["8.24","Medium",8592]
["8.25","Very High",8593]
["8.26","High",8594]
["8.27","Medium",8595]
["8.28","Medium",8596]
["8.29","High",8598]
["8.3","Very High",8571]
["8.30","High",8599]
["8.31","High",8600]
["8.32","Low",8601]
["8.33","Medium",8602]
["8.34","High",8603]
["8.35","Medium",8604]
["8.36","Medium",8605]
["8.37","High",8607]
["8.38","Medium",8608]
["8.39","Medium",8609]
["8.4","Medium",8572]
["8.40","High",8610]
["8.41","Medium",8611]
["8.42","Medium",8612]
["8.43","Very High",8613]
["8.44","High",8615]
["8.45","High",8616]
["8.46","Very High",8617]
["8.47","Very High",8618]
["8.48","Medium",8619]
["8.49","High",8620]
["8.5","Very High",8573]
["8.50","Medium",8621]
["8.51","Low",8622]
["8.52","Low",8623]
["8.53","Low",8624]
["8.54","High",8625]
["8.55","Low",11182]
["8.56","Medium",11183]
["8.57","Medium",11184]
["8.58","High",11185]
["8.59","High",11186]
["8.6","Medium",8574]
["8.60","High",11187]
["8.61","Medium",11188]
["8.62","Very High",11189]
["8.63","High",11190]
["8.64","Medium",11191]
["8.65","Low",11192]
["8.66","High",11193]
["8.67","High",11194]
["8.68","High",11195]
["8.69","Medium",11196]
["8.7","High",8575]
["8.70","Medium",11197]
["8.71","Very High",11198]
["8.72","Medium",11199]
["8.73","Medium",11200]
["8.74","High",11201]
["8.75","Medium",11202]
["8.76","Medium",11203]
["8.77","Medium",11204]
["8.78","Medium",11205]
["8.79","Medium",11206]
["8.8","Medium",8576]
["8.80","Medium",11207]
["8.81","Low",11208]
["8.82","Medium",11209]
["8.83","Low",11210]
["8.84","Low",11211]
["8.85","Medium",11212]
["8.86","Medium",11213]
["8.87","Medium",11214]
["8.88","Low",11215]
["8.89","High",11216]
["8.9","High",8577]
["8.90","High",11217]
["8.91","High",11218]
["8.92","Medium",11219]
["8.93","Low",11220]
["8.94","Low",11221]
["8.95","Medium",11222]
["8.96","Medium",11223]
["8.97","Low",11224]
["8.98","High",11225]
["8.99","Medium",11226]
["9.1","Low",8390]
["9.10","Medium",8399]
["9.11","Medium",8400]
["9.12","Medium",8401]
["9.13","Low",8402]
["9.14","Medium",8403]
["9.15","Medium",8404]
["9.16","High",8405]
["9.17","High",8406]
["9.18","Low",8407]
["9.19","Low",8408]
["9.2","Very High",8391]
["9.20","Medium",8409]
["9.21","Medium",8410]
["9.22","Low",8411]
["9.23","Low",8412]
["9.24","Medium",8413]
["9.25","Low",8414]
["9.26","Low",8415]
["9.27","Low",8416]
["9.28","Medium",8417]
["9.29","Low",8418]
["9.3","Very High",8392]
["9.4","High",8393]
["9.5","High",8394]
["9.6","Low",8395]
["9.7","Medium",8396]
["9.8","Medium",8397]
["9.9","Medium",8398]
["9.99","High",8419]

{"sheet":"Equipment_list","index":7,"n_rows":28,"n_cols":3,"rows_kept":28,"cut":false,"hidden":true,"merged":[]}
["TITLE","Equipment_list_description","ID"]
["Accommodation",null,12]
["Cargo Mach.",null,13]
["Critical Equip.",null,16]
["Deck - Machinery",null,18]
["Deck - Mooring Machinery",null,15]
["Deck - Pipe / Fittings",null,20]
["Documentation",null,21]
["E/R - Air Comp.",null,8]
["E/R - Aux. Engine",null,4]
["E/R - Aux. Mach.",null,7]
["E/R - Boiler",null,5]
["E/R - Main Engine",null,3]
["E/R - Pipes/ valves & fittings",null,9]
["E/R - Pumps",null,32]
["E/R - Purifier",null,6]
["Elect. Mach. & Equip.",null,10]
["Hull & Tanks",null,19]
["Inert Gas",null,14]
["LSA / FFA",null,17]
["Miscellaneous",null,22]
["Navigation - DGPS / EPFS / AIS",null,28]
["Navigation - ECDIS",null,25]
["Navigation - Echo Sounder / Speed Log",null,26]
["Navigation - GMDSS & Communication",null,23]
["Navigation - Others",null,11]
["Navigation - RADAR",null,24]
["Navigation - VDR / BNWAS",null,30]

{"sheet":"PSC_MOU","index":8,"n_rows":11,"n_cols":3,"rows_kept":11,"cut":false,"hidden":true,"merged":[]}
["TITLE","PSC_MOU_description","ID"]
["Asia and the Pacific",null,2]
["Caribbean",null,4]
["Europe and the North Atlantic",null,1]
["Latin America",null,3]
["The Black Sea region",null,6]
["The Indian Ocean",null,8]
["The Mediterranean",null,7]
["The Riyadh MoU",null,9]
["USCG",null,10]
["West and Central Africa",null,5]

{"sheet":"Inspection_type","index":9,"n_rows":13,"n_cols":2,"rows_kept":13,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Bunkering Audit",14]
["Cargo Audit",17]
["Engineering Audit",16]
["ISM Audit",2]
["ISPS Audit",3]
["IT Audit",10]
["MLC Audit",1]
["Mooring Audit",9]
["Nav Audit / Verification",8]
["Onboard Training",18]
["Ship Staff Insp.",15]
["Suptd. Insp.",13]

{"sheet":"Deficiency_Cause","index":10,"n_rows":8,"n_cols":3,"rows_kept":8,"cut":false,"hidden":true,"merged":[]}
["TITLE","Deficiency_Cause_description","ID"]
["Behaviour Based",null,1]
["Equipment Related",null,4]
["External Factors",null,5]
["Human Error",null,7]
["Inappropriate Procedure",null,8]
["Industry Issue",null,6]
["Knowledge Based",null,3]

{"sheet":"Observer_code","index":11,"n_rows":3,"n_cols":3,"rows_kept":3,"cut":false,"hidden":true,"merged":[]}
["TITLE","Observer_code_description","ID"]
["Owner / Marine / Tech. Suptd.",null,3]
["Ship Staff",null,2]

{"sheet":"Status_code","index":12,"n_rows":6,"n_cols":3,"rows_kept":6,"cut":false,"hidden":true,"merged":[]}
["TITLE","Status_code_description","ID"]
["Completed",null,6]
["Deferred to D D",null,5]
["In progress",null,3]
["Not Started",null,2]
["Waiting spare",null,4]

{"sheet":"PSC_ref_no","index":13,"n_rows":19,"n_cols":2,"rows_kept":19,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Alarms",9]
["Cargo operations including equipment",7]
["Certificates & Documentation",2]
["Dangerous Goods",13]
["Emergency Systems",5]
["Fire safety",8]
["ISM",16]
["ISPS",17]
["Life saving appliances",12]
["MLC, 2006",18]
["Other",19]
["Pollution Prevention",15]
["Propulsion and auxiliary machinery",14]
["Radio communication",6]
["Safety of Navigation",11]
["Structural condition",3]
["Water/Weathertight condition",4]
["Working and Living Conditions",10]

{"sheet":"Risk_value_of_obs","index":14,"n_rows":1,"n_cols":2,"rows_kept":1,"cut":false,"hidden":true,"merged":[]}
["Risk Value of observation","ID"]

{"sheet":"Year","index":15,"n_rows":18,"n_cols":1,"rows_kept":18,"cut":false,"hidden":true,"merged":[]}
["Year"]
[2014]
[2015]
[2016]
[2017]
[2018]
[2019]
[2020]
[2021]
[2022]
[2023]
[2024]
[2025]
[2026]
[2027]
[2028]
[2029]
[2030]

{"sheet":"Month","index":16,"n_rows":13,"n_cols":1,"rows_kept":13,"cut":false,"hidden":true,"merged":[]}
["Month"]
["Jan"]
["Feb"]
["Mar"]
["Apr"]
["May"]
["Jun"]
["Jul"]
["Aug"]
["Sep"]
["Oct"]
["Nov"]
["Dec"]

{"sheet":"Date_","index":17,"n_rows":32,"n_cols":1,"rows_kept":32,"cut":false,"hidden":true,"merged":[]}
["Date"]
["01"]
["02"]
["03"]
["04"]
["05"]
["06"]
["07"]
["08"]
["09"]
[10]
[11]
[12]
[13]
[14]
[15]
[16]
[17]
[18]
[19]
[20]
[21]
[22]
[23]
[24]
[25]
[26]
[27]
[28]
[29]
[30]
[31]

{"sheet":"Sheet1","index":18,"n_rows":24,"n_cols":6,"rows_kept":24,"cut":false,"hidden":true,"merged":[]}
[]
[null,"ID","E",null,"Date Recorded",1]
[null,"UNIQUE ID","F",null,"Type of Deficiency",2]
[1,"Date Recorded","G",null,"Observer code",3]
["ignore","Vessel Type","H",null,"Type of Inspection",4]
[null,"Internal / External","I",null,"Description of Deficiency",5]
[null,"Drydock","J",null,"Equipment Categories",6]
[null,"Information Sharing","K",null,"Area of Observation",7]
[null,"Critical_item","L",null,"Deficiency Cause",8]
[null,"Deficiency Type","M",null,"VIQ Ref Number",9]
[null,"Deficiency Cause","N",null,"Risk Value of Obs",10]
[null,"Inspection Type","O",null,"PSC Ref Number",11]
[null,"Equipments","P",null,"PSC MOU ID",12]
[null,"VIQ Reference Number","Q",null,"Action Taken or Required",13]
[null,"Risk Value of the observation","R",null,"Target Date",14]
[null,"PSC Reference Number","S",null,"PO Ref No.",15]
[null,"PSC MOU","T",null,"Status Code",16]
[null,"Observer Code","U",null,"Date Completed",17]
[null,"Target Date","V",null,"Drydock",18]
[null,"Status Code","W",null,"Info Sharing",19]
[null,"Description of Deficiency","X",null,"Critical Item Flag",20]
[null,"Action taken / required","Y",null,"Audit Type",21]
[null,"PO ref no","Z"]
[null,"Date completed","AA"]

{"sheet":"Ship_information","index":19,"n_rows":2,"n_cols":4,"rows_kept":2,"cut":false,"hidden":true,"merged":[]}
["Ship_ID","Ship_Name","FILE_NAME","Export_Date"]
["53","DHT PUMA (24-08-2023)","53_1693270933291.xlsm","2024-01-01 01:01:10"]

{"sheet":"External_Deficiency_type","index":20,"n_rows":5,"n_cols":3,"rows_kept":5,"cut":false,"hidden":true,"merged":[]}
["TITLE","Type of deficiency_description","ID"]
["Condn of Class / Memo",null,5]
["Defect",null,1]
["Non Conformity",null,2]
["Observation",null,3]

{"sheet":"External_Inspection_type","index":21,"n_rows":11,"n_cols":2,"rows_kept":11,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Cargo Audit",17]
["Flag State Insp.",5]
["ISM Audit",2]
["ISPS Audit",3]
["MLC Audit",1]
["Nav Audit / Verification",8]
["OM Insp. (Eg. SIRE / CDI etc.)",6]
["Others (Eg. Insurance etc.)",12]
["PSC Inspection",4]
["Terminal Insp.",11]

{"sheet":"External_Observer_code","index":22,"n_rows":7,"n_cols":3,"rows_kept":7,"cut":false,"hidden":true,"merged":[]}
["TITLE","Observer_code_description","ID"]
["Class Surveyor",null,4]
["FSC Inspector",null,5]
["Others (Eg. Insurance etc.)",null,9]
["PSC Insp.",null,6]
["SIRE / CDI Insp.",null,8]
["Terminal Insp.",null,7]

{"sheet":"Sheet Version","index":23,"n_rows":2,"n_cols":2,"rows_kept":2,"cut":false,"hidden":true,"merged":[]}
["Version","Title"]
["2.0","Version 2.0"]