{"text_format":"1","workbook":"xlsx","n_sheets":24,"sheets":["Mainsheet","Completed","Calc","Areaofobs","Vessel_type","Deficiency_type","VIQrefno","Equipment_list","PSC_MOU","Inspection_type","Deficiency_Cause","Observer_code","Status_code","PSC_ref_no","Risk_value_of_obs","Year","Month","Date_","Sheet1","Ship_information","External_Deficiency_type","External_Inspection_type","External_Observer_code","Sheet Version"],"not_rendered":{"charts":0,"images":1,"macros":1,"external_links":0,"defined_names":12,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Mainsheet","index":0,"n_rows":39,"n_cols":28,"rows_kept":39,"cut":false,"hidden":false,"merged":[[10,8,10,9],[10,12,10,13],[12,6,12,27],[8,6,8,27]]}
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,"Defect - Damage Monitoring Sheet"]
[]
[null,null,null,null,null,null,null,"Date of Report","16-Mar-2024",null,null,"Ship Name","DHT SUNDARBANS (05-12-2023)"]
[]
[null,null,null,null,null,null,"VERSION : 2.0"]
[]
[]
[]
[null,null,null,"ID","SHIPSIDE UNIQUEID","UNIQUE ID","Date Recorded","Type of Deficiency","Observer code","Type of Inspection","Description of Deficiency","Equipment Categories","Area of Observation","Deficiency Cause","VIQ Ref Number","Risk Value of Obs","PSC Ref Number","PSC MOU ID","Action Taken or Required","Target Date","PO Ref No.","Status Code","Date Completed","Drydock","Info Sharing","Critical Item","Audit Type","Superintendent Remarks"]
[null,null,null,null,81664,"0_Wed Jun 15 2022 02:48:19 GMT+0800","2022-11-04T08:00:00","Defect","Ship Staff","Ship Staff Insp.","WHRS soot blow not possible from ECR panel.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Spares received and installed on 23 November 2023 by service engineer. System could not be tried out in presence of service engineer with ME stopped.\nSystem tried out at sea but found no response from ECR control as well as from local control panel. Communication with office and maker in progress. Presently, soot blow of EGB is carried out from local control panel. ","2024-03-31T08:00:00","SSUN230029","In progress",null,"No","No","No","Internal","Service attendance will be planned when vessel calls Singapore "]
[null,null,null,null,39736,"55_Mon Sep 12 2022 14:27:41 GMT+0800","2022-11-08T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Various electrical panels in vessel without indications, due faulty indicator lamp unit and faulty winding heater timer","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","11.10","Medium","","","The indication lamps are faulty and hence raised required spares. ","2024-03-31T08:00:00","SSUN230018","Waiting spare",null,"No","No","No","Internal","Spares will be supplied in Singapore "]
[null,null,null,null,88297,"0_Fri Apr 28 2023 05:18:03 GMT+0800","2023-04-19T08:00:00","Defect","Ship Staff","Ship Staff Insp.","APT PEAK BALLAST LINE TRO UNIT PCB AND FILTER BY PASS VALVE PCB DEFFECTIVE.","E/R - Pipes/ valves & fittings","Cargo / Ballast Systems","Equipment Related","8.8","Medium","","","AFT peak ballast line TRO unit PCB and Filter Bypass Vavle PCB is defective. Its not operational and its under GC claims.","2024-03-31T08:00:00","SSUN230013","Waiting spare",null,"No","No","No","Internal"]
[null,null,null,null,32504,"55_Fri Jun 02 2023 10:15:42 GMT+0800","2023-05-19T08:00:00","Defect","Ship Staff","Ship Staff Insp.","The EGCS Scrubber Absorber Bottom plate has a minor crack at the welding seam.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Cold Repair was carried out inside the Scrubber Absorber and additional Support was fitted to avoid Flexing of bottom plate, kept under close monitioring. Defect kept open till further instructions from Office /maker. Leak is under observation. ","2024-03-31T08:00:00","","In progress",null,"No","No","No","Internal"]
[null,null,null,null,89089,"55_Tue Sep 19 2023 16:20:13 GMT+0800","2023-07-03T08:00:00","Observation","Ship Staff","Ship Staff Insp.","Rust spots have been observed on the accommodation and funnel / EGCS casing","Accommodation","General Appearance","External Factors","","","","","Accommodation block derusting and maintenance has been completed and maintenance on EGCS casing is to be done.","2024-03-31T08:00:00","","In progress",null,"No","No","No","Internal","job must be prioritized "]
[null,null,null,null,12077,"55_Fri Sep 01 2023 11:56:50 GMT+0800","2023-07-09T08:00:00","Defect","Ship Staff","Ship Staff Insp.","JCW Controller Valve has leakage from control valve Gland.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Attending job will require a Suitable Anchorage and Require ME/AE Stopping-Blackout job-Leak temporarily controlled by tightening-but leakage varies at different position of valve controller. ","2024-03-31T08:00:00","","Not Started",null,"No","No","No","Internal"]
[null,null,null,null,69208,"55_Thu Aug 24 2023 00:27:07 GMT+0800","2023-08-17T08:00:00","Breakdown,Defect","Ship Staff","Ship Staff Insp.","Leak Noticed from Top End of Actuator for Draught Gauge Valve Port Side ","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","","","","","Vessel manual does not have valve specication in detail. Vessel sent email to office to  request assistance to identify parts to be ordered from Hanla.","2024-03-31T08:00:00","","In progress",null,"No","No","No","Internal","Has the vessel raised RO for this item? "]
[null,null,null,null,85428,"55_Fri Sep 15 2023 09:51:22 GMT+0800","2023-08-31T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Main engine Start air pipe for No.6 Unit is holed","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.1","Medium","","","Start Air pipe was removed and repairs carried out by welding.  Presently its working fine. Received spare pipe. Awaiting suitable anchorage to carry out the job","2024-03-31T08:00:00","SSUN230177","Not Started",null,"No","No","No","Internal"]
[null,null,null,null,50174,"55_Fri Sep 29 2023 00:20:55 GMT+0800","2023-09-22T08:00:00","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Main engine Turbocharger Suction casing trunk -room -grating are rusted.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Vessel will plan this at suitable anchorage when ME Stopped and attend to carry out derusting -cleaning-painting of Trunk -room and floor gratings.","2024-03-31T08:00:00","","In progress",null,"No","No","No","Internal"]
[null,null,null,null,97379,"55_Fri Sep 29 2023 00:44:12 GMT+0800","2023-09-22T08:00:00","Observation","Ship Staff","Ship Staff Insp.","Various Air trunkings in Engine room-IG Blower platform, BWTS Room, Near Aux boiler 2-Staircase needs to be repaired-Including flap for IG Blower Air trunk.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.18","High","","","Vessel  attempted IG b lower Platform air trunking. It was wasted in middle. Same patched up with cold repair and its working fine.  Vessel will attempt for Boiler Area and BWTS platform at the earliest oppurtunity. ","2024-03-31T08:00:00","","In progress",null,"No","No","No","Internal"]
[null,null,null,null,62270,"55_Fri Sep 29 2023 00:15:19 GMT+0800","2023-09-26T08:00:00","Observation","Ship Staff","Ship Staff Insp.","EGCS Sealing air fan-B had excessive vibration-Motor Bearing Housing worn and causing wobble in shaft and excessive vibration","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Sealing Air fan motor- bearing housing was built up by cold work, temporarily made sealing fan operational. Spare Motor on order","2024-03-31T08:00:00","SSUN 230187","Waiting spare",null,"No","No","No","Internal"]
[null,null,null,null,18623,"55_Fri Oct 20 2023 14:39:07 GMT+0800","2023-10-09T08:00:00","Defect","Ship Staff","Ship Staff Insp.","FWG No 1 distillate pump not building up sufficient pressure. ","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.3","Medium","","","Pump opened up for overhauling and found wear ring out of limit and needs to be renewed.  No spare available onboard. Requisition raised for new spares. Presently, No.1 FWG is not in use. ","2024-03-31T08:00:00","DSUN230197","Waiting spare",null,"No","No","No","Internal","Spares on order, will be connected once ready."]
[null,null,null,null,42250,"55_Mon Nov 20 2023 15:01:01 GMT+0800","2023-11-15T08:00:00","Defect","Ship Staff","Ship Staff Insp.","No 1 Control air dryer compressor not building up discharge pressure.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.30","High","","","Initial trouble reported was compressor not building up discharge pressure, vessel received spare compressor under PO SSUN230130, same installed in place. After installation system charged and checked for leakages. No leaks found on external pipes/connections. Leak suspected in condenser or evaporator coil which is difficult to identify and fix onboard. As per last mail, office will be supplying complete new unit. Details sent through mail. \n","2024-03-31T08:00:00","PO SSUN235077","Waiting spare",null,"No","No","No","Internal","Complete new control air dryer on order."]
[null,null,null,null,20768,"55_Thu Nov 30 2023 12:54:05 GMT+0800","2023-11-25T08:00:00","Observation","Ship Staff","Ship Staff Insp.","Port windlass Hydraulic cylinder for brake engaging and disengaging is leaking.","Deck - Machinery","Mooring","Equipment Related","9.20","Medium","","","Requisition raised for the spare parts PO DSUN230199. ","2024-03-31T08:00:00","PO DSUN230199 ","Waiting spare",null,"No","No","No","Internal","Spares on order."]
[null,null,null,null,34967,"55_Thu Nov 30 2023 12:58:15 GMT+0800","2023-11-25T08:00:00","Observation","Ship Staff","Ship Staff Insp.","Stbd windlass Hydraulic cylinder for brake engaging and disengaging is leaking.","Deck - Machinery","Mooring","Equipment Related","9.20","Medium","","","Requisition raised for the spare parts PO DSUN230199. ","2024-03-31T08:00:00","PO DSUN230199 ","Waiting spare",null,"No","No","No","Internal","Spares on order."]
[null,null,null,null,75652,"55_Thu Jan 11 2024 16:11:56 GMT+0800","2024-01-02T08:00:00","Defect","Ship Staff","Ship Staff Insp.","NO.2 TG VACUUM PUMP NOT DEVELOPING VACCUM IN CONDENSOR","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.30","High","","","TG vacuum pump is operational but not developing vacuum  in the condensor. As there is no spares for overhaul,  Spares has been raised for the same.  ","2024-03-31T08:00:00","SSUN240016","Waiting spare",null,"No","No","No","Internal"]
[null,null,null,null,84147,"55_Thu Jan 11 2024 16:17:18 GMT+0800","2024-01-11T08:00:00","Defect","Ship Staff","Ship Staff Insp.","NO.1 IG BLOWER MOTOR FAN BROKEN ","","Cargo / Ballast Systems","Equipment Related","","","","","Presently, blower motor is cooled via ducting and its operational. As there is no spare onboard, requisition has been raised. ","2024-03-31T08:00:00","SSUN240031","Waiting spare",null,"No","No","No","Internal"]
[null,null,null,null,36472,"55_Wed Feb 28 2024 07:12:52 GMT+0800","2024-02-27T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Pin hole at 2 locations on 2 pipe sections which is below the water line in ballast condition in Galley Overboard Pipeline. ","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Temporary the leaks are arrested by water activating tape and hose clip. Leak under observation. Office concurrence in progress. ","2024-03-31T08:00:00","","In progress",null,"No","No","No","Internal"]
[null,null,null,null,71033,"55_Wed Feb 28 2024 07:22:01 GMT+0800","2024-02-27T08:00:00","Defect","Ship Staff","Ship Staff Insp.","The cladding on the EGB has been wasted at various locations near HP and Superheater header leading to leakage of exhaust gas during sailing. ","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Temporary the cladding is patched up with new lagging material and GI sheet followed by taping it. Suspect the leak is from the plate inside the EGB casing. Office concurrence in progress","2024-03-31T08:00:00","","In progress",null,"No","No","No","Internal"]
[null,null,null,null,15287,"55_Wed Feb 28 2024 07:24:04 GMT+0800","2024-02-26T08:00:00","Defect","Ship Staff","Ship Staff Insp.","The pH sensor water container has a pin hole on the top cover. ","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.11","Medium","","","Presently its patched up with cold repair and is in working condition. Awaiting spare for the same. ","2024-03-31T08:00:00","SSUN240066","Waiting spare",null,"No","No","No","Internal"]
[null,null,null,null,91895,"55_Sat Mar 02 2024 11:00:27 GMT+0800","2024-02-29T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Both LO purifier heaters Temperature Controller is erractic","E/R - Purifier","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Presently the purifier temperature is maintained manually and its working condition. Investigation in progress to check the controllers. ","2024-05-02T08:00:00","","In progress",null,"No","No","No","Internal"]
[null,null,null,null,99418,"55_Sat Mar 16 2024 00:01:40 GMT+0800","2024-03-06T08:00:00","Defect,Observation","Ship Staff","Ship Staff Insp.","During routine rounds found  noise emanating from main engine lo purifier motor .","E/R - Purifier","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Same opened up for inspection ,found centrifugal clutch , driver and clutch pulley worn out in way of  bearing seating area .  overhauled with shims and new bearings, but found slight improvement .  RO SSUN240071 raised . same has been stopped  and kept stand by.","2024-06-15T08:00:00","SSUN240071","Waiting spare",null,"No","No","No","Internal"]

{"sheet":"Completed","index":1,"n_rows":248,"n_cols":28,"rows_kept":248,"cut":false,"hidden":false,"merged":[[10,8,10,9],[10,12,10,13],[12,6,12,27],[8,6,8,27]]}
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,"Defect - Damage Monitoring Sheet"]
[]
[null,null,null,null,null,null,null,"Date of Report","16-Mar-2024",null,null,"Ship Name","DHT SUNDARBANS (05-12-2023)"]
[]
[null,null,null,null,null,null,"VERSION : 2.0"]
[]
[]
[]
[null,null,null,"ID","SHIPSIDE UNIQUEID","UNIQUE ID","Date Recorded","Type of Deficiency","Observer code","Type of Inspection","Description of Deficiency","Equipment Categories","Area of Observation","Deficiency Cause","VIQ Ref Number","Risk Value of Obs","PSC Ref Number","PSC MOU ID","Action Taken or Required","Target Date","PO Ref No.","Status Code","Date Completed","Drydock","Info Sharing","Critical Item","Audit Type","Superintendent Remarks"]
[null,null,null,24453,null,"55_20/3/2022 4:39:59 pm","2022-01-21T23:59:35","Defect","Ship Staff","Ship Staff Insp.","ME JCW Temperature Control Valve Position Sensor Fail\t\t\t\t","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.2","Low","","","We have replaced the valve positioner and alarm has cleared.","2022-05-16T23:59:35","SSUN220038","Completed","2022-05-21T23:59:35","No","No","No","Internal"]
[null,null,null,26352,50895,"55_Tue Jul 12 2022 02:02:45 GMT+0800","2022-02-01T23:59:35","Observation","Ship Staff","Ship Staff Insp.","VDR RCU UNIT PCB Eject button defective, New PCB received & replaced but due to Error in installation, Old one placed back in use again as per Instructions from office. New MCB on board. However New MCB onboard need to be configured for all channels inputs and that only service engineer can do. ","Navigation - Others","Navigation","Equipment Related","4.7","High","","","Awaiting service Engineer attendance. Office to be informed prior convenient port call for attendance of service Engineer.  So that new PCB onboard can be programmed for all input channels and can be fixed.\n06 Sep 2022 / Action Taken - New PCB installed. Remote troubleshooting and programming carried out by Service Engineer. Eject button & VDR working in good order . Job Completed.","2022-10-11T23:59:35","N/A - Office to be informed prior convenient port call for attendance of service Engineer. ","Completed","2022-08-19T23:59:35","No","No","No","Internal"]
[null,null,null,26354,34778,"55_Tue Jul 12 2022 02:16:00 GMT+0800","2022-02-01T23:59:35","Critical Equipment","Ship Staff","Ship Staff Insp.","ECDIS fitted onboard 2 x JRC 901-B AND USED AS PRIMARY MEANS OF Navigation SSD last replaced July 2022. \nNo spare Pre-Programmed SSD's onboard as required under critical spare part list of company.","Navigation - ECDIS","Navigation","Equipment Related","","","","","Spare pre programmed SSD's not required , since As per the all makers, if vessel is equipped with dual ECDIS, no additional spares to be maintained.","2022-10-11T23:59:35","","Completed","2022-09-19T23:59:35","No","No","No","Internal"]
[null,null,null,24351,null,"55_1/3/2022 4:26:07 am","2022-02-06T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Engine room skylight mooring wire found to have broken strands.","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","Equipment Related","5.47","Medium","","","Wire replaced.","2022-04-17T23:59:35","","Completed","2022-03-02T23:59:35","No","No","No","Internal"]
[null,null,null,24352,null,"55_5/3/2022 9:43:01 pm","2022-02-06T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Various tap fittings in accomodation found to be leaking as reported by crew in Safety meeting","Accommodation","MLC Related","Equipment Related","11.13","Low","","","Requistion received through SSUN220050 and leaking taps renewed.","2022-05-08T23:59:35","","Completed","2022-03-31T23:59:35","No","No","No","Internal"]
[null,null,null,24353,null,"55_6/3/2022 1:50:14 pm","2022-02-07T23:59:35","Defect","Ship Staff","Ship Staff Insp.","FCV 1211 is not operating by remotely. Drive motor for the same was burnt. Currently FCV 1211 is operated manually.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","6.21","High","","","Drive motor received, job completed. ","2022-11-29T23:59:35","SSUN220035","Completed","2022-09-21T23:59:35","No","No","No","Internal","Raise requisition for drive motor ASAP."]
[null,null,null,24354,null,"55_6/3/2022 2:31:27 pm","2022-02-07T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Port and stbd accommodation ladder lashing guide are not in good condition (rubber guides on which wire lashing is resting).","Deck - Pipe / Fittings","General Appearance","Equipment Related","5.47","Medium","","","Lashing guide ordered and received on board.\nSame has been renewed. Job completed.\n","2022-05-07T23:59:35","","Completed","2022-04-20T23:59:35","No","No","No","Internal","Noted. Close defect after renewing same."]
[null,null,null,24350,null,"55_5/3/2022 10:03:02 pm","2022-02-08T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Electrical insulation matt found to be missing at various panels in Engine room.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.24","Low","","","Electrical insulation matt at missing locations installed.","2022-03-10T23:59:35","","Completed","2022-02-26T23:59:35","No","No","No","Internal","Mat supplied at DD. Close defect after putting at missing area."]
[null,null,null,24355,null,"55_5/3/2022 9:33:12 pm","2022-02-08T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Loose items in Engine room not secured.","Miscellaneous","Eng. / Strg. Comp.","External Factors","5.11","Low","","","All loose items have been be shifted to their respective stowage  proper location and secured.","2022-03-08T23:59:35","","Completed","2022-02-18T23:59:35","No","No","No","Internal","Noted."]
[null,null,null,24356,null,"55_5/3/2022 9:47:01 pm","2022-02-08T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Various doors including accomodation and purifier room door the holding latches screw found to be missing.","Accommodation,E/R - Purifier","Safety / LSA / FFA","Equipment Related","5.35","Medium","","","Missing screw for latches installed and door closing function tested for proper closing.","2022-04-08T23:59:35","","Completed","2022-02-22T23:59:35","No","No","No","Internal","Noted."]
[null,null,null,24357,null,"55_5/3/2022 9:50:37 pm","2022-02-08T23:59:35","Critical Equipment,Observation","Ship Staff","Ship Staff Insp.","Critical spare parts found to be missing and also critical spare part inventory to be updated in PAL.","E/R - Main Engine,Elect. Mach. & Equip.","Emgcy. Systems","Equipment Related","10.13","Very High","","","Missing critical spare parts to be requested upon taking complete inventory of critical spare parts. Closing as all spares ordered from vessel as well approved by office","2022-05-10T23:59:35","SSUN220007,SSUN220015,SSUN220016,SSUN220017,SSUN220018,SSUN220019,SSUN220020,SSUN220021,SSUN220022,S","Completed","2022-03-30T23:59:35","No","No","No","Internal"]
[null,null,null,24358,null,"55_5/3/2022 9:55:52 pm","2022-02-08T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Laundry drying room thermostat not cutting off.","Accommodation","MLC Related","Equipment Related","11.14","Medium","","","Thermostat received and installed. job completed.","2022-04-30T23:59:35","SSUN220034","Completed","2022-04-30T23:59:35","No","No","No","Internal","Raise requisition."]
[null,null,null,24359,null,"55_5/3/2022 9:59:53 pm","2022-02-08T23:59:35","Observation","Ship Staff","Ship Staff Insp.","EGCS side shell renewal and various stubb piece renewed in Engine room and same area needs to be derusted and painting including funnel top deck plate.","Hull & Tanks","Structural Condn. / WT integrity ","Equipment Related","10.31","Very High","","","Area needs to be derusted and painted.","2022-03-10T23:59:35","","Completed","2022-02-23T23:59:35","No","No","No","Internal","Noted."]
[null,null,null,24360,null,"55_5/3/2022 10:07:37 pm","2022-02-08T23:59:35","Other","Ship Staff","Ship Staff Insp.","ECA Book not available onboard.","Miscellaneous","MARPOL Related","Industry Issue","10.5","Low","","","ECA book received and updated","2022-04-10T23:59:35","","Completed","2022-03-26T23:59:35","No","No","No","Internal"]
[null,null,null,24361,null,"55_5/3/2022 10:25:49 pm","2022-02-08T23:59:35","Defect","Ship Staff","Ship Staff Insp.","WHRS cladding insulation material found to be missing and same needs to be installed.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.19","Very High","","","yard fabricated insulation cladding cover and given to ship, same installed in place.","2022-04-10T23:59:35","Waiting for the engine to be stopped for enabling installation.","Completed","2022-03-31T23:59:35","No","No","No","Internal"]
[null,null,null,24362,null,"55_5/3/2022 10:33:34 pm","2022-02-08T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Scrubber room not fitted with engine room alarm extension.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.2","Low","","","Alarm signal light and cable procured in DD and same installed. Tested operation and found satisfactory.","2022-04-15T23:59:35","","Completed","2022-04-15T23:59:35","No","No","No","Internal","Noted."]
[null,null,null,24363,null,"55_5/3/2022 10:42:44 pm","2022-02-08T23:59:35","Defect","Ship Staff","Ship Staff Insp.","High pressure pipe connected upon completion of decarb not secured with antisplash tape.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.19","Very High","","","Potential areas of splash to be protected with anti splash tape same installed and completed.","2022-04-09T23:59:35","","Completed","2022-03-31T23:59:35","No","No","No","Internal"]
[null,null,null,24454,null,"55_20/3/2022 2:53:05 pm","2022-02-09T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Reported Garbage Compactor not opertional","Deck - Machinery","General Appearance","Equipment Related","6.2","High","","","NEW GARBAGE COMPACTOR INSTALLED","2022-09-10T23:59:35","SSUN220040","Completed","2022-09-20T23:59:35","No","No","No","Internal"]
[null,null,null,24455,null,"55_20/3/2022 4:53:22 pm","2022-02-09T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Fault alarm was received on ER OMD Panel for Boiler Area #2","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.35","Medium","","","Spares received and same replaced and job completed.","2022-05-12T23:59:35","SSUN220039","Completed","2022-05-21T23:59:35","No","No","No","Internal"]
[null,null,null,25518,16952,"55_Tue May 31 2022 08:20:33 GMT+0800","2022-02-09T23:59:35","Defect","Ship Staff","Ship Staff Insp.","AUX DG TC COMPRESSOR WHEEL FOUND CHIPPED , EFFICIENCY OF TC NOT RELIABLE","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","SPARE TC CARTRIDGE REQUESTED. SAME INSTALLED","2022-05-12T23:59:35","STAI150016/2","Completed","2022-05-01T23:59:35","No","No","No","Internal"]
[null,null,null,24457,null,"55_20/3/2022 3:10:00 pm","2022-02-10T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Bosun store water mist system repeater panel on bridge showing no indication.\t","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.35","Medium","","","PCB received and renewed.","2022-06-14T23:59:35","SSUN220032","Completed","2022-05-21T23:59:35","No","No","No","Internal"]
[null,null,null,24456,null,"55_20/3/2022 4:17:31 pm","2022-02-13T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Back-up UPS for S-Band RADAR and Fire Fighting CO2 system was operational\t\t\t","LSA / FFA,Navigation - RADAR","Navigation","Equipment Related","","","","","Both UPS was bypassed to make the system online, S band radar spares received and installed. Awaiting spare for Co2 ups.\nNEW UPS RECEIVED installed","2022-09-10T23:59:35","SSUN220036","Completed","2022-09-27T23:59:35","No","No","No","Internal"]
[null,null,null,24842,null,"55_31/3/2022 11:02:04 am","2022-02-26T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Fault with fire detection system due to faulty short circuit isolator.","Critical Equip.,LSA / FFA","Eng. / Strg. Comp.","Equipment Related","5.39","Very High","","","Informed office and the electrical department provided short circuit isolator in singapore on 27/03/2022 same installed and found fault alarm is clear.","2022-04-22T23:59:35","","Completed","2022-03-09T23:59:35","No","No","No","Internal"]
[null,null,null,24839,null,"55_31/3/2022 12:56:19 pm","2022-03-05T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Topping up generator monthly outines tried out, noticed sw valve not holding as well one of the flame sensor is faulty.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","8.25","Very High","","","SW valve renewed.","2022-07-07T23:59:35","","Completed","2022-03-28T23:59:35","No","No","No","Internal"]
[null,null,null,24840,null,"55_31/3/2022 11:11:35 am","2022-03-10T23:59:35","Critical Equipment,Defect","Ship Staff","Ship Staff Insp.","Navigational light control panel though all lights were of “ON” indication without alarms in the panel.but, actually in real scenario no navigational lights present in mast head in monkey island,fwd mast, side light and stern lights.","Navigation - Others","Navigation","Equipment Related","4.8","Medium","","","New panel received & Renewed - tested & working in good order. Job Completed","2022-09-10T23:59:35","New panel received & Renewed - tested & working in good order. Job Completed","Completed","2022-08-18T23:59:35","No","No","No","Internal"]
[null,null,null,24841,null,"55_31/3/2022 1:00:09 pm","2022-03-10T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Port side provision controller display had no indications, though there is no display indications the functionality of the crane controller is in good order. ","Miscellaneous","Structural Condn. / WT integrity ","Equipment Related","8.5","Very High","","","Controller replaced and job completed.","2022-07-17T23:59:35","","Completed","2022-04-02T23:59:35","No","No","No","Internal"]
[null,null,null,25513,83707,"55_Tue May 03 2022 22:23:29 GMT+0800","2022-03-12T23:59:35","Defect","Ship Staff","Ship Staff Insp.","MAIN ENGINE FUEL OIL HEATER #2 FOUND LEAKING ","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.1","Medium","","","FUEL OIL HEATER STACK REMOVED AND GASKET CHANGED,","2022-04-15T23:59:35","","Completed","2022-04-12T23:59:35","No","No","No","Internal"]
[null,null,null,25512,62197,"55_Sun May 01 2022 14:10:21 GMT+0800","2022-03-26T23:59:35","Observation","Ship Staff","Ship Staff Insp.","No 1 ME Fuel pump high pressure pipe connection found to have minor leaks","E/R - Main Engine,E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","High pressure pipe disconnected and found one O-ring to be damaged.  Same replaced and assembled back observed to find leakage to be stopped.","2022-05-06T23:59:35","","Completed","2022-04-09T23:59:35","No","No","No","Internal"]
[null,null,null,25510,18580,"55_Sun May 01 2022 16:40:06 GMT+0800","2022-04-11T23:59:35","Defect","Ship Staff","Ship Staff Insp.","ME DGU CAN A FAILURE","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.1","Medium","","","Service engineer attended in San Diego.  All CAN A and CAN B connections were swapped in E25 box. DGU AL module was replaced. issue rectified.","2022-07-12T23:59:35","SSUN225090","Completed","2022-05-21T23:59:35","No","No","No","Internal"]
[null,null,null,25519,13882,"55_Tue May 31 2022 08:22:47 GMT+0800","2022-04-11T23:59:35","Critical Equipment","Ship Staff","Ship Staff Insp.","SCRUBBER ROOM FIRE DAMPER HARD TO OPERATE","LSA / FFA","Eng. / Strg. Comp.","Equipment Related","5.35","Medium","","","DAMPER TO OVERHAUL AND MAKE FREE TO OPERATE","2022-05-11T23:59:35","","Completed","2022-05-10T23:59:35","No","No","No","Internal"]
[null,null,null,25514,57835,"55_Thu May 26 2022 12:19:35 GMT+0800","2022-04-12T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Doppler log repeater display on Bridge front not clearly readable / visible  in the day-light with maximum brilliance. ","Navigation - Echo Sounder / Speed Log","Navigation","Equipment Related","4.7","High","","","New display ordered and replaced.","2022-04-30T23:59:35","SSUN225078","Completed","2022-04-28T23:59:35","No","No","No","Internal"]
[null,null,null,25515,51330,"55_Thu May 26 2022 12:29:39 GMT+0800","2022-04-12T23:59:35","Observation","Ship Staff","Ship Staff Insp.","MF/ HF Ariel securing clamp was observed missing during monthly test/checks of the equipment as per PMS schedule.","Navigation - GMDSS & Communication","Navigation","Equipment Related","4.7","High","","","MF/ HF Ariel securing clamp renewed.","2022-04-15T23:59:35","","Completed","2022-04-13T23:59:35","No","No","No","Internal"]
[null,null,null,26353,38287,"55_Tue Jul 12 2022 02:08:58 GMT+0800","2022-04-15T23:59:35","Observation","Ship Staff","Ship Staff Insp.","AIS is Unable to switch to LOW TX power (As Required by ISGOTT & Local port requirements)","Navigation - DGPS / EPFS / AIS","Navigation","Equipment Related","4.7","High","","","AIS software updated by shore on team viewer and AIS can be switched to LOW power .","2022-10-11T23:59:35","N/A","Completed","2022-07-16T23:59:35","No","No","No","Internal"]
[null,null,null,25517,66428,"55_Fri May 27 2022 03:16:27 GMT+0800","2022-04-20T23:59:35","Defect","Ship Staff","Ship Staff Insp.","4C COT overfill alarm not operational.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.14","Very High","","","Requisition made for Magnet in float assembly.\nReceived magnet and same has been renewed.\nOverfill alarm operational, job completed.\n","2022-05-01T23:59:35","SSUN220051","Completed","2022-04-29T23:59:35","No","No","No","Internal"]
[null,null,null,25516,71133,"55_Fri May 27 2022 02:52:35 GMT+0800","2022-04-25T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Analyze pump internal leakage alarm on Pump room fixed gas detection system.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.46","Very High","","","Analyze Pump overhauled and renewed flow switch. Job completed. \nNo alarm on Pump room fixed gas detection system \n","2022-04-29T23:59:35","","Completed","2022-04-28T23:59:35","No","No","No","Internal"]
[null,null,null,25511,61845,"55_Tue May 31 2022 08:24:42 GMT+0800","2022-05-03T23:59:35","Defect","Ship Staff","Ship Staff Insp.","#1 FWG EJECTOR NOZZLE WORN, SHELL TEMP HIGH DUE TO LESS VACUUM","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","ejector renewed.\nvacuum is good now with fwg production 25mt","2022-09-11T23:59:35","SSUN220096","Completed","2022-09-17T23:59:35","No","No","No","Internal"]
[null,null,null,25509,70470,"55_Tue May 31 2022 08:26:30 GMT+0800","2022-05-04T23:59:35","Defect,Observation","Ship Staff","Ship Staff Insp.","WHRS MANHOLE GASKETS HAVE LEAK. THREADS FOR SECURING STUDA DAMGED","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Manhole gaskets renewed on WHRS for 6 no doors.","2022-08-04T23:59:35","","Completed","2022-05-25T23:59:35","No","No","No","Internal"]
[null,null,null,25633,61687,"55_Wed Jun 15 2022 02:20:34 GMT+0800","2022-05-13T23:59:35","Defect","Ship Staff","Ship Staff Insp.","M/E Tachometer no 1 and no 2 showing eratic reading when engine stopped.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","TACHOMETER CONNECTIONS RE CHECKED AND MADE CORRECT SAME WORKING.","2022-09-11T23:59:35","SSUN220058","Completed","2022-09-24T23:59:35","No","No","No","Internal"]
[null,null,null,25634,89448,"0_Wed Jun 15 2022 02:26:06 GMT+0800","2022-05-13T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Common rail box tested for cracks and found few cracks and action needs to be taken.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Crack end punched in order to arrest the cracks.","2022-08-13T23:59:35","","Completed","2022-06-01T23:59:35","No","No","No","Internal"]
[null,null,null,25846,28192,"55_Mon Jun 20 2022 21:19:50 GMT+0800","2022-05-17T23:59:35","Defect","Ship Staff","Ship Staff Insp.","During the pressure testing it was observed that the Cargo Line No. 3 to IG Connection T-Piece was leaking. Same was fully tightened up and the leak was stopped.\nHowever suspect the Cargo Line No. 3 Valve to IG Line (OD-339) is suspected to be leaking. The line was re-pressurized to 11.0 bars and confirmed no leaks were observed during the time of inspection.\n","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.11","Medium","","","Renewed seat ring of valve OD-339, job completed.","2022-06-10T23:59:35","","Completed","2022-06-01T23:59:35","No","No","No","Internal"]
[null,null,null,25635,92117,"55_Wed Jun 15 2022 02:29:09 GMT+0800","2022-05-21T23:59:35","Observation","Ship Staff","Ship Staff Insp.","WIO sensor installed along with BWMS is decommissioned. Need to install new type WIO sensor.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Office to follow up to supply new type Water in oil sensor. once received same to be installed and an mimic in aconis to be created with aconis engineer.","2022-09-20T23:59:35","","Completed","2022-09-16T23:59:35","No","No","No","Internal"]
[null,null,null,25636,73085,"0_Wed Jun 15 2022 02:30:41 GMT+0800","2022-05-21T23:59:35","Defect","Ship Staff","Ship Staff Insp.","M/E top brazing no 4 is leaking.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","M/E top brazing no 4 needs to be overhauled. Spares are already onboard.","2022-08-21T23:59:35","","Completed","2022-07-08T23:59:35","No","No","No","Internal"]
[null,null,null,25637,81536,"55_Wed Jun 15 2022 02:33:24 GMT+0800","2022-05-21T23:59:35","Observation","Ship Staff","Ship Staff Insp.","M/E ICO lube 440 volt low insulation alarm comes when started.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Isolation transformer has been supplied to vessel and pending installation, same needs to be installed to clear alarm// ","2022-08-21T23:59:35","","Completed","2022-05-31T23:59:35","No","No","No","Internal"]
[null,null,null,25639,47889,"0_Wed Jun 15 2022 02:40:16 GMT+0800","2022-05-21T23:59:35","Defect","Ship Staff","Ship Staff Insp.","EGCS gas analyzer has chopper motor failure alarms","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Communication with maker spare parts ordered.. Gas analyser and service attendance arranged through SSUN225094","2022-09-20T23:59:35","SSUN225094","Completed","2022-09-14T23:59:35","No","No","No","Internal"]
[null,null,null,25641,49623,"0_Wed Jun 15 2022 02:53:28 GMT+0800","2022-05-21T23:59:35","Defect","Ship Staff","Ship Staff Insp.","We have noticed quantity discrepancy with Bilge guard flowmeter.\nTotal quantity discharged overboard recorded in Bilge guard is less than the actual quantity pumped overboard. We are recording actual quantity in ORB with reference to our manual sounding.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","QUANTITIES ARE CHECKED DURING LAST OPERATIONS AND FOUND NOT MUCH DIFFERENCE, UNDER MONITORING.","2023-06-18T23:59:35","SSUN230037","Completed","2023-06-10T23:59:35","No","No","No","Internal"]
[null,null,null,25642,72855,"55_Wed Jun 15 2022 05:05:16 GMT+0800","2022-05-21T23:59:35","Defect","Ship Staff","Ship Staff Insp.","One of the cargo pressure transmitter local display not visible.\n\n","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.41","Medium","","","Pressure transmitter for cargo manifold ordered through SSUN220071 SAME REPLACED AND SYSTEM BACK TO NORMAL","2022-09-17T23:59:35","SSUN220071","Completed","2022-09-25T23:59:35","No","No","No","Internal"]
[null,null,null,25643,11488,"55_Wed Jun 15 2022 05:11:11 GMT+0800","2022-05-21T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Rosemount WSU one of the CPU has failed same ordered and awaiting spare SSUN225084. Communication with maker in progress backup file sent to maker as per request","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.70","Medium","","","Troubleshooting steps taken as per  service technician , Both WSU of Rosemount working satisfactorily","2022-08-21T23:59:35","","Completed","2022-08-06T23:59:35","No","No","No","Internal"]
[null,null,null,25644,95612,"0_Wed Jun 15 2022 05:13:49 GMT+0800","2022-05-21T23:59:35","Defect","Ship Staff","Ship Staff Insp.","IGG firing but having flame failure alarm, flame eye requested, suspect the control valves now, still not succeeded.","E/R - Aux. Mach.","Cargo / Ballast Systems","Equipment Related","10.32","Very High","","","IGG FLAME EYE RENWED TRIED OUT , FOUND SATISFACTORY.","2022-09-20T23:59:35","SSUN220098","Completed","2022-09-20T23:59:35","No","No","No","Internal"]
[null,null,null,25828,97126,"55_Thu Jun 23 2022 19:59:40 GMT+0800","2022-05-26T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Manhole covers on deck to de rust especially areas near the tightening nuts.","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.3","Medium","","","De rusting / painting of Manhole covers on deck  Completed","2022-08-26T23:59:35","","Completed","2022-08-06T23:59:35","No","No","No","Internal"]
[null,null,null,25829,83555,"55_Thu Jun 23 2022 20:31:42 GMT+0800","2022-05-26T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Spot rust and weeping marks observed on Slop P & S Steam manifold.","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.3","Medium","","","De rusting and painting  carried out at Slop P & S Steam manifold.","2022-06-25T23:59:35","","Completed","2022-06-10T23:59:35","No","No","No","Internal"]
[null,null,null,25830,74907,"55_Thu Jun 23 2022 21:01:20 GMT+0800","2022-05-26T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Spot rust and weeping marks observed on COT, WBT Tank domes and Hydraulic valve boxes especially near the Butterfly nuts.","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.3","Medium","","","Spot rust and weeping marks observed on COT, WBT Tank domes and Hydraulic valve boxes especially near the Butterfly nuts completed , ","2022-08-26T23:59:35","","Completed","2022-08-06T23:59:35","No","No","No","Internal"]
[null,null,null,25831,86922,"55_Thu Jun 23 2022 21:27:26 GMT+0800","2022-05-26T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Spot rust and weeping marks observed on Deck pipelines near the supports, U Clamps and flanges.","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.4","Very High","","","Spot de rusting and painting on deck pipelines near the supports, U Clamps and flanges completed","2022-08-26T23:59:35","","Completed","2022-08-19T23:59:35","No","No","No","Internal"]
[null,null,null,25832,16683,"55_Thu Jun 23 2022 19:14:14 GMT+0800","2022-05-26T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","SWL not marked on pad eye in Pump room .","Deck - Pipe / Fittings","General Appearance","Human Error","8.50","Medium","","","SWL marked on pad eyes in pump room.","2022-06-10T23:59:35","","Completed","2022-06-01T23:59:35","No","No","No","Internal"]
[null,null,null,25833,62282,"55_Thu Jun 23 2022 19:20:58 GMT+0800","2022-05-26T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","1 no Garbage bin in Hospital and 1 no in Crew Messroom is not color coded as per Garbage management plan ","Accommodation","General Appearance","Human Error","6.20","Medium","","","Garbage bin in Hospital and Crew Messroom color coded and labelled as per Garbage management plan.","2022-06-10T23:59:35","","Completed","2022-05-29T23:59:35","No","No","No","Internal"]
[null,null,null,25834,35875,"55_Thu Jun 23 2022 19:25:47 GMT+0800","2022-05-26T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Cleaning equipment’s kept in pipe and duct space to remove.","Accommodation","General Appearance","Human Error","11.8","Low","","","Removed cleaning equipment, which kept in pipe and duct space and Notice posted.","2022-06-01T23:59:35","","Completed","2022-05-29T23:59:35","No","No","No","Internal"]
[null,null,null,25835,47274,"55_Thu Jun 23 2022 19:30:52 GMT+0800","2022-05-26T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","All Duty officers to be familiarized with the BWTS and procedures to be posted.","Documentation","Cargo / Ballast Systems","Human Error","6.21","High","","","Familiarisation carried out  regarding BWTS procedure and same has been posted in CCR.","2022-06-10T23:59:35","","Completed","2022-05-30T23:59:35","No","No","No","Internal"]
[null,null,null,25836,34729,"55_Thu Jun 23 2022 19:35:45 GMT+0800","2022-05-26T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Locking pin for Lifebuoys on Deck to be checked for free movement as some of them are painted over.","LSA / FFA","Safety / LSA / FFA","Human Error","5.31","High","","","De rusting and painting of Locking pin of life buoys carried out.\nConfirmed free movement of the same.\n","2022-06-02T23:59:35","","Completed","2022-06-01T23:59:35","No","No","No","Internal"]
[null,null,null,25837,31362,"55_Thu Jun 23 2022 19:52:11 GMT+0800","2022-05-26T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Spare Vapor manifold reducers kept in Midship stores to check for compliance with requirements of OCIMF.","Deck - Machinery","Cargo / Ballast Systems","Equipment Related","8.42","Medium","","","12’ o clock stud pcs were missing for spare vapor manifold reducer.\nNew stud pcs fabricated for the same as per OCIMF requirement. \n","2022-06-10T23:59:35","","Completed","2022-05-31T23:59:35","No","No","No","Internal"]
[null,null,null,25838,46331,"55_Thu Jun 23 2022 20:39:26 GMT+0800","2022-05-26T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","All PV Valves vacuum side wire mesh having Rust spots and stains.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.21","High","","","PV valve vacuum side wire mesh renewed with new wire mesh. ","2022-06-25T23:59:35","","Completed","2022-06-01T23:59:35","No","No","No","Internal"]
[null,null,null,25839,18806,"55_Fri Jun 24 2022 00:30:38 GMT+0800","2022-05-26T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","All lifting gears on Deck to be tagged and marked as per the inventory.","Deck - Machinery","General Appearance","Human Error","8.50","Medium","","","Lifting gear tagged as per the inventory.","2022-06-15T23:59:35","","Completed","2022-06-01T23:59:35","No","No","No","Internal"]
[null,null,null,25840,64245,"55_Fri Jun 24 2022 00:45:50 GMT+0800","2022-05-26T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","No wire lashing for Heavy equipment and stores in Port midship store.","Deck - Machinery","General Appearance","Human Error","5.11","Low","","","Wire lashing taken for heavy equipment in Port midship store.","2022-06-10T23:59:35","","Completed","2022-05-31T23:59:35","No","No","No","Internal"]
[null,null,null,25841,70941,"55_Thu Jun 23 2022 19:08:43 GMT+0800","2022-05-26T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Railing near WBP 2 on bottom platform in Pump room not secured (Bolts loose and some missing).","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","Equipment Related","5.11","Low","","","Railing near WBP 2 on bottom platform in Pump room secured with Bolts and nuts & tighten.","2022-06-10T23:59:35","","Completed","2022-05-29T23:59:35","No","No","No","Internal"]
[null,null,null,25842,17680,"55_Fri Jun 24 2022 00:50:26 GMT+0800","2022-05-26T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Max stowage line for Sprinkler not marked in Sample locker.","LSA / FFA","Safety / LSA / FFA","Human Error","5.48","Medium","","","Max stowage line for Sprinkler marked in Sample locker.","2022-06-10T23:59:35","","Completed","2022-06-01T23:59:35","No","No","No","Internal"]
[null,null,null,25843,36644,"55_Fri Jun 24 2022 18:34:08 GMT+0800","2022-05-26T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","2 nos Safety harness in Stbd midship store in poor condition.","LSA / FFA","Safety / LSA / FFA","Human Error","5.5","Low","","","2 Safety harness kept in stbd mid ship store were not in use, same has been removed from stbd midship store and discarded. Safety harness with two lanyard, two snap hooks and an energy absorber kept in mid ship store.","2022-06-02T23:59:35","","Completed","2022-05-30T23:59:35","No","No","No","Internal"]
[null,null,null,26355,73012,"55_Tue Jul 12 2022 02:26:34 GMT+0800","2022-05-26T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Bridge wing control console speed log repeater not readable with max brilliance in the day light time.","Navigation - Echo Sounder / Speed Log","Navigation","Equipment Related","","","","","After cleaning contactors of cables and restarting Bridge wing control console speed log repeater panel clearly visible","2022-10-11T23:59:35","","Completed","2022-07-12T23:59:35","No","No","No","Internal"]
[null,null,null,25844,33742,"55_Fri Jun 24 2022 00:00:04 GMT+0800","2022-05-26T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","All portable ladders on Deck not tagged and inventory not maintained.","Deck - Machinery","General Appearance","Human Error","8.50","Medium","","","All portable ladders on Deck tagged and inventory maintained for the same","2022-06-15T23:59:35","","Completed","2022-06-04T23:59:35","No","No","No","Internal"]
[null,null,null,25845,83648,"55_Thu Jun 23 2022 19:42:03 GMT+0800","2022-05-26T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Locking pin for Hook of Stbd davit in Sunken deck and Bosun store davit is frozen.","Deck - Machinery","Safety / LSA / FFA","Equipment Related","8.50","Medium","","","Locking pin for Hook of Stbd davit in Sunken deck and Bosun store davit greased and confirmed free movement.","2022-06-10T23:59:35","","Completed","2022-06-04T23:59:35","No","No","No","Internal"]
[null,null,null,25847,12387,"55_Fri Jun 24 2022 18:46:13 GMT+0800","2022-05-26T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Bilge cover for Aft Bilge well near Propeller shaft on port side is missing.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Human Error","10.15","Low","","","Bilge cover for Aft Bilge well near Propeller shaft to be put back in position.","2022-06-15T23:59:35","","Completed","2022-05-31T23:59:35","No","No","No","Internal"]
[null,null,null,25848,27902,"55_Fri Jun 24 2022 18:51:21 GMT+0800","2022-05-26T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Max stowage line for Sprinkler not marked in Chemical locker.","LSA / FFA","Safety / LSA / FFA","Human Error","5.48","Medium","","","Max stowage line for Sprinkler to be marked in Chemical locker.","2022-06-10T23:59:35","","Completed","2022-06-01T23:59:35","No","No","No","Internal"]
[null,null,null,26503,33172,"55_Sun Aug 14 2022 19:29:02 GMT+0800","2022-07-17T23:59:35","Observation","Ship Staff","Ship Staff Insp.","WHRS BELLOW AT LP SECTION PORT SIDE HOLED","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","BLAST FURNANCE CEMENT APPLIED ON HOLE","2022-10-16T23:59:35","","Completed","2022-09-01T23:59:35","No","No","No","Internal"]
[null,null,null,26647,22681,"55_Wed Aug 31 2022 18:05:11 GMT+0800","2022-08-03T23:59:35","Defect","Ship Staff","Ship Staff Insp.","It was observed that the Loadicator display was not coming. The CPU was restarted and it was observed that there is no output signal to the display ,also that the CPU processor fan upon restarting was cutting in and off continuously & no output through the terminal ports  .Suspect motherboard malfunction  .","Miscellaneous","Cargo / Ballast Systems","Equipment Related","9.7","Medium","","","Received new CPU with preloaded loadicator software ","2022-09-17T23:59:35","","Completed","2022-09-15T23:59:35","No","No","No","Internal"]
[null,null,null,26646,46817,"55_Wed Aug 31 2022 17:58:20 GMT+0800","2022-08-11T23:59:35","Defect","Ship Staff","Ship Staff Insp.","STBD WINDLASS SPLIT DRUM BUSH HAS BEEN DISLOCATED FROM PLACE CAUSING UNDUE NOISE AND WOBBLE OF SPLIT DRUM.","Deck - Machinery","Mooring","Equipment Related","9.14","Medium","","","Sleeve bearing of stbd windlass drum renewed.","2023-02-18T23:59:35","SSUN220193","Completed","2023-02-09T23:59:35","No","No","No","Internal"]
[null,null,null,26780,36264,"55_Tue Sep 13 2022 16:19:07 GMT+0800","2022-08-14T23:59:35","Defect","Ship Staff","Ship Staff Insp.","16K/8.5K Steam Control Valve Positioner does not feed back values to AMS ","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","11.10","Medium","","","New spare positioner received & replaced","2022-11-13T23:59:35","SSUN220192","Completed","2022-11-02T23:59:35","No","No","No","Internal"]
[null,null,null,26785,75506,"55_Wed Sep 14 2022 16:30:35 GMT+0800","2022-08-14T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Auto-Telephone for bridge, CO2 room, elevator machinery room was not operational due faulty unit and PCB","Elect. Mach. & Equip.","Communication","Equipment Related","10.11","Medium","","","ALL MENTIONED TELEPHONES MADE OPERATIONAL","2022-11-13T23:59:35","SSUN220194\nSSUN220111","Completed","2022-09-20T23:59:35","No","No","No","Internal"]
[null,null,null,26786,42025,"55_Thu Sep 15 2022 17:45:32 GMT+0800","2022-08-15T23:59:35","Defect","Ship Staff","Ship Staff Insp.","VISCOSENSOR VALVE PASSING, NO MAINTENANCE CAN BE CARRIED OUT ON VISCOSENSOR.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","VESSEL TO DO MAINTENANCE WHILE ON MGO.\nVALVES TO BE ORSERED IN NEXT BUDGET","2022-11-14T23:59:35","SSUN220189","Completed","2022-09-14T23:59:35","No","No","No","Internal"]
[null,null,null,26787,63197,"55_Thu Sep 15 2022 17:43:34 GMT+0800","2022-08-15T23:59:35","Defect","Ship Staff","Ship Staff Insp.","MAIN COPT/CSW PUMP DISCHARGE VALVE HAS DAMAGED SLEEVE CAUSING NRV VALVE NOT FUNCTIONING AND PUMP ROTATING ANTICLOCKWISE\n","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","EXISTING VALVE GUIDE REBULIT AND PUT IN PLACE SAME WORKING GOOD.","2022-11-14T23:59:35","","Completed","2022-10-01T23:59:35","No","No","No","Internal"]
[null,null,null,26779,25214,"55_Mon Sep 12 2022 16:54:21 GMT+0800","2022-08-18T23:59:35","Defect","Ship Staff","Ship Staff Insp.","CONTROL AIR DRYER #1 COMPRESSOR IS HAVING FAULTY TEMP SENSOR FOR COMPRESSOR","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","NEW COMPRESSOR INSTALLED , UNIT WORKING IN GOOD CONDITION.","2022-11-17T23:59:35","SSUN220209","Completed","2022-09-23T23:59:35","No","No","No","Internal"]
[null,null,null,26777,41981,"55_Wed Sep 07 2022 21:47:08 GMT+0800","2022-08-20T23:59:35","Defect","Ship Staff","Ship Staff Insp.","#2 COPT Over speed relay malfunction, causing the turbine to trip at 50 to 100 rpm","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","10.32","Very High","","","Replaced with new spare received Singapore Transit","2022-11-12T23:59:35","SSUN220201","Completed","2022-11-03T23:59:35","No","No","No","Internal"]
[null,null,null,26781,25126,"55_Tue Sep 13 2022 16:35:00 GMT+0800","2022-08-21T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Manifold pressure transmitter printer drive unit faulty","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.41","Medium","","","Renewed printer drive unit.","2022-11-20T23:59:35","SSUN220208","Completed","2022-11-04T23:59:35","No","No","No","Internal"]
[null,null,null,26782,15461,"55_Tue Sep 13 2022 17:36:26 GMT+0800","2022-08-21T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Ballast Tank VRCS valve indicator unit transmitter value was fluctuating","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","Required spare,\nSPARES RECEIVED and job completed","2023-01-19T23:59:35","SSUN220204","Completed","2022-12-29T23:59:35","No","No","No","Internal"]
[null,null,null,26784,41234,"55_Wed Sep 14 2022 16:23:30 GMT+0800","2022-08-26T23:59:35","Defect","Ship Staff","Ship Staff Insp.","While trying out Anemometer alarms, only visual alarm was working, horn was not operational and the unit was also giving ESB 220 VAC Low Insulation alarm","Elect. Mach. & Equip.","Communication","Equipment Related","5.9","Very High","","","Spares received-Job completed","2022-11-25T23:59:35","SSUN220220","Completed","2022-11-11T23:59:35","No","No","No","Internal"]
[null,null,null,27153,12242,"55_Wed Sep 21 2022 09:42:16 GMT+0800","2022-08-27T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Stbd windlass operating lever hydraulic block, found leaking","Deck - Machinery","Mooring","Equipment Related","9.14","Medium","","","job completed with onboard spares RO raised to maintain ROB","2022-11-14T23:59:35","SSUN220118","Completed","2022-10-19T23:59:35","No","No","No","Internal"]
[null,null,null,27162,31454,"55_Wed Sep 21 2022 10:25:54 GMT+0800","2022-08-27T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Magnetic compass dimmer AC dimmer switch not operational.","Navigation - Others","Navigation","Equipment Related","4.7","High","","","Vessel rcvd spares at Singapore on 10th Nov 2022.  Same has been renewed.\nMagnetic compass dimmer AC dimmer switch is operational now.","2022-11-19T23:59:35","SSUN220184","Completed","2022-11-01T23:59:35","No","No","No","Internal"]
[null,null,null,27163,58309,"55_Fri Sep 23 2022 15:21:44 GMT+0800","2022-08-27T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Pressure gauge from central cooler blackened, glycerin needs renewal","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Same renewed","2022-09-07T23:59:35","","Completed","2022-08-24T23:59:35","No","No","No","Internal"]
[null,null,null,27164,44385,"55_Fri Sep 23 2022 15:25:11 GMT+0800","2022-08-27T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Missing Limit switch valve plate for APT valves","E/R - Pumps","Eng. / Strg. Comp.","Industry Issue","","","","","Plates fabricated and installed in place","2022-11-23T23:59:35","","Completed","2022-08-26T23:59:35","No","No","No","Internal"]
[null,null,null,27165,30876,"55_Wed Sep 21 2022 09:49:15 GMT+0800","2022-08-27T23:59:35","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Main deck port & stbd side aft of manifold area to be de rusted","Deck - Pipe / Fittings","General Appearance","External Factors","11.3","Medium","","","Main deck port and stbd side spot chipping / painting completed","2022-10-05T23:59:35","","Completed","2022-09-12T23:59:35","No","No","No","Internal"]
[null,null,null,27166,12508,"55_Wed Sep 21 2022 10:14:26 GMT+0800","2022-08-27T23:59:35","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Main deck cargo pipelines and associated valves in front of pumproom entry bulkhead de rusting / spot painting required.","Deck - Pipe / Fittings","General Appearance","External Factors","11.4","Very High","","","Main deck cargo pipelines and associated valves in front of pumproom entry bulkhead de rusted and spot painting carried out","2022-09-20T23:59:35","","Completed","2022-08-25T23:59:35","No","No","No","Internal"]
[null,null,null,27167,83173,"55_Wed Sep 21 2022 10:18:32 GMT+0800","2022-08-27T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Deck fixed foam system line drain in foam room was found having minor leak, drain valve to be renewed or overhauled and fixed back.","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.35","Medium","","","Deck fixed foam system line drain in foam room will be overhauled","2022-08-27T23:59:35","","Completed",null,"No","No","No","Internal"]
[null,null,null,27168,69229,"55_Wed Sep 21 2022 09:47:29 GMT+0800","2022-08-27T23:59:35","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Pumproom entrance weather tight door stbd side rubber packing to be renewed","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.6","Medium","","","Rubber packing of stbd side pumproom entrance door adjusted properly and is properly sitting in watertight groove of weather tight door","2022-09-20T23:59:35","","Completed","2022-09-08T23:59:35","No","No","No","Internal"]
[null,null,null,27170,16722,"55_Wed Sep 21 2022 09:52:04 GMT+0800","2022-08-27T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Shackles used for Anchor lashings were found having less SWL (4 Tones)  than required, as the Anchors are weighing 17.25 tones.","Deck - Mooring Machinery","Mooring","External Factors","9.2","Very High","","","Anchor lashing shackles replaced with appropriate size shackles of 17 tons","2022-10-04T23:59:35","SSUN-220168 – DECK STORES","Completed","2022-09-16T23:59:35","No","No","No","Internal"]
[null,null,null,27177,11450,"55_Wed Sep 21 2022 10:08:21 GMT+0800","2022-08-27T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Vessel does not have wire slings/shackles of appropriate SWL for testing the hose handling crane to required Load using the Load Cell.","","Cargo / Ballast Systems","Equipment Related","8.5","Very High","","","Load testing of both midship cranes carried out .Both midship cranes load tested to 20 Tons using load cell","2022-10-04T23:59:35","SUN-220168 – DECK STORES","Completed","2022-09-23T23:59:35","No","No","No","Internal"]
[null,null,null,27178,85901,"55_Fri Sep 23 2022 15:27:55 GMT+0800","2022-08-27T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Soft patch found on aft hydraulic inlet water line.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.31","Very High","","","New pipe fabricated and installed in place","2022-09-13T23:59:35","","Completed","2022-09-05T23:59:35","No","No","No","Internal"]
[null,null,null,27179,63124,"55_Wed Sep 21 2022 10:16:33 GMT+0800","2022-08-27T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Stbd Lifeboat Self-Lowering remote control wire roller sheave blocks were found having slight chaffing and same needs to be renewed with new brass blocks.","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.28","Very High","","","Stbd side lifeboat self lowering controller wire sheaves renewed with brass sheaves","2022-10-04T23:59:35","SSUN220190","Completed","2022-09-24T23:59:35","No","No","No","Internal"]
[null,null,null,27180,39256,"55_Wed Sep 21 2022 09:44:49 GMT+0800","2022-08-27T23:59:35","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Helicopter landing area collapsible railings spot de rusting requiring and to be highlighted","Deck - Pipe / Fittings","General Appearance","External Factors","11.3","Medium","","","Helicopter landing area collapsible railings spot de rusting and painting / highlighting completed","2022-10-05T23:59:35","","Completed","2022-09-24T23:59:35","No","No","No","Internal"]
[null,null,null,27181,60055,"55_Wed Sep 21 2022 10:12:36 GMT+0800","2022-08-27T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Paint locker sprinkler system drain valve leaking same to be overhauled.","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.35","Medium","","","Paint locker sprinkler system drain valve overhauled","2022-09-13T23:59:35","","Completed","2022-08-22T23:59:35","No","No","No","Internal"]
[null,null,null,27182,35572,"55_Wed Sep 21 2022 10:23:52 GMT+0800","2022-08-27T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Course recorder marking / printing observed faded during routine inspection. Spare set of Stylus has been ordered. Stylus adjusted presently.","Navigation - Others","Navigation","Equipment Related","4.7","High","","","Course recorder stylus replaced with new one . Working satisfactorily","2022-11-19T23:59:35","SSUN220152","Completed","2022-09-18T23:59:35","No","No","No","Internal"]
[null,null,null,27156,80155,"55_Sun Oct 02 2022 10:41:14 GMT+0800","2022-09-13T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","EGCS JET SECTION SW INLET PIPE STUB PIECE TO BE RENEWED","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","VESSEL AWAITNG SPARES, PRESENTLY REMOVED PIPE AND BUILD UP FOR THE HOLED SECTION HAS BEEN CARRIED OUT, SAME PRESSURE TESTED AND PUT IN USE AND PRESNETLY NOT LEAKING .","2023-01-13T23:59:35","SSUN220216","Completed","2022-12-23T23:59:35","No","No","No","Internal"]
[null,null,null,27157,10918,"55_Sun Oct 02 2022 10:53:16 GMT+0800","2022-09-13T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","HP drum safety valve to be renewed. Spare safety valve supplied to vessel.","E/R - Boiler","Eng. / Strg. Comp.","External Factors","10.32","Very High","","","HP DRUM SV HAS PITTING ON VALVE SEAT SAME WILL BE RENEWED AT NEXT AVALABLE OPPURTUNITY..","2022-12-13T23:59:35","","Completed","2022-10-03T23:59:35","No","No","No","Internal"]
[null,null,null,27158,54326,"55_Sun Oct 02 2022 10:54:20 GMT+0800","2022-09-13T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Sludge collecting tank steam heating valve leaking. Same to be renewed","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Valve to be renewed once vessel changes over to MGO .\n","2022-12-13T23:59:35","","Completed","2022-10-02T23:59:35","No","No","No","Internal"]
[null,null,null,27159,85971,"55_Sun Oct 02 2022 10:52:01 GMT+0800","2022-09-13T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Funnel deck floor need chipping and painting. Special paint supplied for this to be used.","Miscellaneous","General Appearance","Equipment Related","11.1","High","","","Funnel deck chipped and re painted.","2023-01-13T23:59:35","","Completed","2023-01-02T23:59:35","No","No","No","Internal"]
[null,null,null,27160,27267,"55_Sun Oct 02 2022 10:56:09 GMT+0800","2022-09-13T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Work shop fire door is bent. Same need renewal.","LSA / FFA","Eng. / Strg. Comp.","Equipment Related","5.14","Very High","","","Replaced with new one","2023-01-13T23:59:35","","Completed","2022-11-14T23:59:35","No","No","No","Internal"]
[null,null,null,27169,27494,"55_Sun Oct 02 2022 10:50:01 GMT+0800","2022-09-13T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","NO.3 ER FAN ROOM CEILING NEEDS REPAIR","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","CEILING HAS FALLEN DOWN FROM SUPPORT. NEW SUPPORT TO BE FABRICATED AND CEILING TO BE SECURED.","2022-12-13T23:59:35","","Completed","2022-09-17T23:59:35","No","No","No","Internal"]
[null,null,null,27171,68393,"55_Sun Oct 02 2022 10:57:18 GMT+0800","2022-09-13T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","S/G bilge drain valve frozen. Same to be overhauled and eased up.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Valve to be dismantled and overhauled.","2022-10-13T23:59:35","","Completed","2022-09-18T23:59:35","No","No","No","Internal"]
[null,null,null,27172,77168,"55_Sun Oct 02 2022 10:44:05 GMT+0800","2022-09-13T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","EGCS DECK HOUSE NEEDS CLEANING","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","CLEANING DONE, PAINTING WILL BE CARRIED OUT PRIOR ARRIVAL PORT","2022-10-13T23:59:35","","Completed","2022-09-17T23:59:35","No","No","No","Internal"]
[null,null,null,27173,42401,"55_Sun Oct 02 2022 10:47:45 GMT+0800","2022-09-13T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","MIST CATCHER IN ER HAS OIL LEAKAGE MARKS. TO BE OPENED AND INSPECTED.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","FLANGES RE TIGHTENED ","2022-10-13T23:59:35","","Completed","2022-09-17T23:59:35","No","No","No","Internal"]
[null,null,null,27174,26780,"55_Sun Oct 02 2022 10:58:03 GMT+0800","2022-09-13T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","EFP room bilge drain valve frozen. Same to be overhauled and eased up.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Valve to be overhauled","2022-10-13T23:59:35","","Completed","2022-09-18T23:59:35","No","No","No","Internal"]
[null,null,null,27175,84071,"55_Sun Oct 02 2022 08:40:53 GMT+0800","2022-09-13T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Port Windlass brake cylinder match marks not aligned. To be adjusted as per maker’s manual procedure. Match marks on both windlass to be highlighted.","Deck - Mooring Machinery","Mooring","Equipment Related","9.20","Medium","","","Port Windlass brake cylinder match marks  aligned and  adjusted as per maker’s manual procedure. Match marks on both windlass highlighted.","2022-11-12T23:59:35","","Completed","2022-09-21T23:59:35","No","No","No","Internal"]
[null,null,null,27176,32584,"55_Sun Oct 02 2022 08:45:21 GMT+0800","2022-09-13T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Port Windlass gear oil to renew.","Deck - Mooring Machinery","Mooring","Equipment Related","9.14","Medium","","","Port Windlass gear oil renewed","2022-10-13T23:59:35","","Completed","2022-09-23T23:59:35","No","No","No","Internal"]
[null,null,null,27360,76799,"55_Tue Oct 18 2022 20:05:01 GMT+0800","2022-10-02T23:59:35","Defect","Ship Staff","Ship Staff Insp.","SHIP'S LAUNDRY WASHING MACHINE NOT OPERATIONAL","Accommodation","MLC Related","Equipment Related","","","","","NEW WASHING MACHINE RECEIVED. JOB COMPLETED","2022-11-14T23:59:35","SSUN220245","Completed","2022-11-14T23:59:35","No","No","No","Internal"]
[null,null,null,29385,54697,"55_Thu Mar 16 2023 00:00:33 GMT+0800","2022-10-04T23:59:35","Non Conformity","Ship Staff","Nav Audit / Verification","Position Plotting Intervals in Singapore Strait was not followed as per ENC Marking.","Navigation - ECDIS","Navigation","Human Error","","","","","All OOWs briefed on the requirements of position verification intervals with instructions / requirements. ","2023-01-03T23:59:35","","Completed","2022-10-30T23:59:35","No","No","No","Internal"]
[null,null,null,29386,12842,"55_Thu Mar 16 2023 00:03:14 GMT+0800","2022-10-04T23:59:35","Non Conformity","Ship Staff","Nav Audit / Verification","Steering Light was found In-operational during Audit Checks. ","Navigation - Others","Navigation","Human Error","","","","","Faulty Steering light fixture replaced with new spare and tried out found working satisfactory.","2023-01-03T23:59:35","","Completed","2022-10-08T23:59:35","No","No","No","Internal","Please discuss this observation and preventive action in next safety meeting/tool box meeting, with the officers/crew involved, to avoid recurrence."]
[null,null,null,29387,19252,"55_Thu Mar 16 2023 00:06:42 GMT+0800","2022-10-04T23:59:35","Non Conformity","Ship Staff","Nav Audit / Verification","Historical Records checked and found that Draft entries from last Disport to Singapore in Deck Log Book was not there. ","Navigation - Others","Navigation","Human Error","","","","","Relevant draft entries made in the deck log books by new bridge team officers and All OOWs briefed about making entries in bridge bell book and deck log books in line with instructions / requirements on regular basis.","2022-10-30T23:59:35","","Completed","2022-10-30T23:59:35","No","No","No","Internal","Please discuss this observation and preventive action in next safety meeting/tool box meeting, with the officers/crew involved, to avoid recurrence."]
[null,null,null,27365,99234,"55_Mon Oct 31 2022 15:45:21 GMT+0800","2022-10-07T23:59:35","Observation","Ship Staff","Ship Staff Insp.","BRIDGE AIR CON BLOWER WOBBLING","Miscellaneous","MLC Related","Equipment Related","","","","","Fan belt replaced and now no wobbling. noticed pulley wheel to have crack same shall be requested from vessel end.","2023-01-06T23:59:35","","Completed","2022-12-22T23:59:35","No","No","No","Internal"]
[null,null,null,27364,29748,"55_Mon Oct 31 2022 15:46:58 GMT+0800","2022-10-13T23:59:35","Observation","Ship Staff","Ship Staff Insp.","ER BLOWERS ON DECK HAS RUST ON BASE AND HINGES","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","Equipment Related","11.4","Very High","","","DE RUSTING  AND PAINTING CARIED OUT.","2022-11-17T23:59:35","","Completed","2022-11-16T23:59:35","No","No","No","Internal"]
[null,null,null,27362,25555,"55_Tue Oct 25 2022 15:00:40 GMT+0800","2022-10-19T23:59:35","Defect","Ship Staff","Ship Staff Insp.","EGCS SCRUBBER PUMP VFD PANEL B PORTABLE AC NOT WORKING DUE TO BURNT PCB FOR DISPLAY","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","Spare received, replaced and rectified.","2023-03-18T23:59:35","","Completed","2023-02-18T23:59:35","No","No","No","Internal","RO no not mentioned in the PO Ref no."]
[null,null,null,27363,17261,"55_Tue Oct 25 2022 14:58:51 GMT+0800","2022-10-19T23:59:35","Defect","Ship Staff","Ship Staff Insp.","WHRS EXHAUST OUTLET SENSOR NO.21 NOT WORKING AND GIVING SENSOR FAIL ALARM","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","WHRS exhaust outlet faulty sensor No. 21 replaced with new, which was received during last call at Singapore","2023-08-13T23:59:35","","Completed","2023-08-04T23:59:35","No","No","No","Internal",""]
[null,null,null,27155,63938,"55_Sun Oct 02 2022 08:48:05 GMT+0800","2022-10-20T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","VRCS piping on deck need de-rusting and painting.","Deck - Pipe / Fittings","General Appearance","External Factors","11.4","Very High","","","VRCS Line Derusting and Painting Completed\n","2023-07-30T23:59:35","","Completed","2023-06-06T23:59:35","No","No","No","Internal"]
[null,null,null,27154,70816,"55_Wed Sep 21 2022 10:10:43 GMT+0800","2022-10-23T23:59:35","Other","Owner / Marine / Tech. Suptd.","Ship Staff Insp.","Accommodation superstructure deck spot de rusting / painting required.","Accommodation","General Appearance","External Factors","11.8","Low","","","Work Aloft on Accommodation Block and Funnel Casing Completed at Anchorage during Port Stay at Cap Lopez, Gabon. All accessible spots in Accommodation Front, Sides, Bridge Wing, Bulwark Supporting Bridge Wing spot de-rusted, primer and final coat completed. ","2023-08-29T23:59:35","","Completed","2023-03-21T23:59:35","No","No","No","Internal"]
[null,null,null,27361,89196,"55_Thu Oct 20 2022 13:53:35 GMT+0800","2022-10-26T23:59:35","Defect","Ship Staff","Ship Staff Insp.","E/R OIL  MIST DETECTOR FOR PURIFIER ROOM FAULTY","LSA / FFA","Eng. / Strg. Comp.","Equipment Related","","","","","SPARES RECEIVED FAULTY DETECTOR REPLACED, WORKING SATISFACTORY.","2023-06-26T23:59:35","SSUN230014","Completed","2023-06-06T23:59:35","No","No","No","Internal","Spares will be supplied at next available opportunity."]
[null,null,null,26357,81857,"55_Mon Aug 01 2022 19:45:51 GMT+0800","2022-10-31T23:59:35","Defect","Ship Staff","Ship Staff Insp.","MAIN ENGINE STBD BRIDGE WING CONSOLE OUT OF ORDER DUE TO BWU09 MODULE NOT OPERATIONAL","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.31","Very High","","","Kongsberg engineer attended all put back to normal . No alarm since singapore.","2023-02-17T23:59:35","","Completed","2023-02-19T23:59:35","No","No","No","Internal","Servicing will be arranged next call Singapore."]
[null,null,null,27161,15694,"55_Tue Oct 04 2022 10:10:35 GMT+0800","2022-11-10T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Loadicator unale to activate online data from rosemount tank gauging online feed system","Miscellaneous","Cargo / Ballast Systems","Equipment Related","9.7","Medium","","","Troubleshooting in progress , office advised regarding the same\nEmerson Technician attended at Singapore on 21 Feb 23, reported, NAPA Technician remote assistance provided and the job is completed now","2023-04-22T23:59:35","","Completed","2023-03-19T23:59:35","No","No","No","Internal"]
[null,null,null,27959,96099,"55_Fri Dec 16 2022 06:54:21 GMT+0800","2022-11-12T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Fwd Catwalk platform got deformed & buckled, also railing of the same platform bent towards outer side, due to heavy weather impact. ","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.3","Medium","","","Straightening of deformed Fwd Catwalk platform and railing done.\n","2022-12-18T23:59:35","","Completed","2022-11-19T23:59:35","No","No","No","Internal"]
[null,null,null,26504,81077,"55_Sun Aug 14 2022 19:39:40 GMT+0800","2022-11-13T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Signal Column at E/R bottom platform . FWD. STBD. not working. Found transformer burnt for same","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","New spare received -PCB-replaced-system unit made operational-tested","2023-07-28T23:59:35","SSUN230019","Completed","2023-07-23T23:59:35","No","No","No","Internal"]
[null,null,null,27956,96804,"55_Fri Dec 16 2022 06:27:01 GMT+0800","2022-11-19T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Support bracket for ME Fuel Supply unit Inlet & Outlet pipe manifold has a crack","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","SUPPORT BRACKET WELDING JOB COMPLETED AFTER OFFICE CONCURRENCE.","2023-04-18T23:59:35","","Completed","2023-04-04T23:59:35","No","No","No","Internal"]
[null,null,null,27957,31172,"55_Fri Dec 16 2022 06:23:06 GMT+0800","2022-11-23T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Pump room Fan No.1 has vibration","Deck - Machinery,Cargo Mach.","Cargo / Ballast Systems","Equipment Related","5.18","High","","","Pump room fan on starboard side found to have excessicve vibration and same attended noticed cover plate on impeller had given off and floating same rectified and now in order.","2022-12-24T23:59:35","SSUN220285","Completed","2022-12-14T23:59:35","No","No","No","Internal"]
[null,null,null,27955,36927,"55_Fri Dec 16 2022 03:41:59 GMT+0800","2022-11-27T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Following COW machine valves were found passing during pressure testing of COW line prior discharge port.\n2P(1 Nos),  2S (1Nos), 3S (1Nos), 4P(1Nos), 1C(2Nos)","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.34","High","","","COW Machine valves Seat Rings renewed. \nWill be rechecked during line pressure testing. ","2023-05-25T23:59:35","SSUN230053.","Completed","2023-03-12T23:59:35","No","No","No","Internal"]
[null,null,null,27958,36802,"55_Fri Dec 16 2022 03:14:29 GMT+0800","2022-11-30T23:59:35","Defect","Ship Staff","Ship Staff Insp.","No.1 & No.2 Foam monitor valve is leaking.","LSA / FFA","Emgcy. Systems","Equipment Related","5.38","High","","","No.2  and No.1 Foam monitor valve replaced, Foam monitor tested, no leak detected.\n","2022-12-17T23:59:35","","Completed","2022-12-02T23:59:35","No","No","No","Internal"]
[null,null,null,27953,68643,"55_Fri Dec 16 2022 03:19:45 GMT+0800","2022-12-02T23:59:35","Defect","Ship Staff","Ship Staff Insp.","No.3 and No.2 Fire line Isolation valve is leaking.","LSA / FFA","Emgcy. Systems","Equipment Related","5.38","High","","","Isolation valves overhauled. Isolation valves tested after overhauling, found in order.","2022-12-17T23:59:35","","Completed","2022-12-16T23:59:35","No","No","No","Internal"]
[null,null,null,27954,56662,"55_Fri Dec 16 2022 03:24:36 GMT+0800","2022-12-02T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Valve between IG line to VECS line cannot be closed properly, presently valve is in open condition and will not cause any problem for discharging operation.","Inert Gas","Cargo / Ballast Systems","Equipment Related","8.30","High","","","Fabricated new key for valve stem and put back the mechanical actuator in position & confirmed valve is opening and shutting properly. \nValve were removed to checked for opening and shutting position. Valve is opening and shutting properly. ","2023-01-19T23:59:35","","Completed","2022-12-28T23:59:35","No","No","No","Internal"]
[null,null,null,26356,45280,"55_Sat Jul 30 2022 09:01:39 GMT+0800","2022-12-04T23:59:35","Defect","Ship Staff","Ship Staff Insp.","VRCS UNLOADER MECHANISM NOT OPERATIONAL","Deck - Machinery","Cargo / Ballast Systems","Equipment Related","8.31","High","","","Unloader switch received at 21/02/2023 and replaced now in order.","2023-03-18T23:59:35","SSUN220141","Completed","2023-03-01T23:59:35","No","No","No","Internal"]
[null,null,null,26783,86098,"55_Tue Sep 13 2022 17:51:37 GMT+0800","2022-12-06T23:59:35","Defect","Ship Staff","Ship Staff Insp.","#1  Economiser Feed Water pump motor, while running observed heavy vibration and abnormal sound, also observed bearing seat was damaged","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Motor received installed tried out and in order now.","2023-03-18T23:59:35","SSUN220182","Completed","2023-02-15T23:59:35","No","No","No","Internal"]
[null,null,null,28142,53498,"0_Fri Dec 30 2022 05:57:24 GMT+0800","2022-12-09T23:59:35","Defect","Ship Staff","Ship Staff Insp.","NO1 CSW PUMP DISCHARGE VALVE NOT HOLDING. IT WAS INFORMED THAT VALVE PARTS WERE FOUND IN LT COOLER.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","All 3 main cooling sea water pump discharge valves leak test carried out and observed No1 cooling sea water discharge valve holding even with the discharge valve open condition (NR valve).\nHowever NO 3 Main cooling sea water pump discharge valve found not holding even with discharge valve completely shut (manually).\nVessel renewed No 3 Main cooling sea water pump discharge valve with new spare.\n","2023-11-29T23:59:35","SSUN230045","Completed","2023-10-12T23:59:35","No","No","No","Internal"]
[null,null,null,28143,97657,"55_Fri Dec 30 2022 05:50:10 GMT+0800","2022-12-09T23:59:35","Defect","Ship Staff","Ship Staff Insp.","HP DRUM GUAGE GLASS LEAKING","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","Guage glass of HP drum was erroded and erroded surface filled up with permatex high temperature and was fitted in place. As of now it is an temporary repair and no leaks.","2023-01-19T23:59:35","SSUN230029","Completed","2023-01-13T23:59:35","No","No","No","Internal","Believe in the mean time you can use high press gaskets."]
[null,null,null,28136,17214,"0_Fri Dec 30 2022 05:59:13 GMT+0800","2022-12-10T23:59:35","Defect","Ship Staff","Ship Staff Insp.","3 way valve of no1 HFO purifier found to be leaking same needs to be renewed,","E/R - Purifier","Eng. / Strg. Comp.","Equipment Related","","","","","3 Way valve for HFO purifier no.1 renewed.","2023-01-19T23:59:35","","Completed","2022-12-24T23:59:35","No","No","No","Internal"]
[null,null,null,28137,14413,"55_Fri Dec 30 2022 06:51:27 GMT+0800","2022-12-10T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Servo oil Filter screen flashing and not readable.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","File taking inventory we found one spare display. Same replaced.","2023-03-10T23:59:35","","Completed","2023-01-10T23:59:35","No","No","No","Internal"]
[null,null,null,28138,53534,"0_Fri Dec 30 2022 06:55:50 GMT+0800","2022-12-10T23:59:35","Defect","Ship Staff","Ship Staff Insp.","STarboard Lifeboat batteries were renewed with old batteries as the batteries in place failed to start.","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","Battery ordered through SSUN230004 received and replaced.","2023-03-17T23:59:35","SSUN230004","Completed","2023-02-14T23:59:35","No","No","No","Internal"]
[null,null,null,28139,97293,"0_Fri Dec 30 2022 06:57:36 GMT+0800","2022-12-10T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Vessel received UPS for CITADEL but our AMS UPS had breakdown and hence we installed CITADEL UPS to AMS.","Miscellaneous","Safety / LSA / FFA","Equipment Related","","","","","Received UPS-Battery- connected to Citadel Communication phone.","2023-09-29T23:59:35","SSUN230007","Completed","2023-09-14T23:59:35","No","No","No","Internal"]
[null,null,null,28141,83230,"0_Fri Dec 30 2022 06:53:45 GMT+0800","2022-12-10T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Accomodation Gas detection system sensors are all expired and give alarm at times and calibration is not accepting many times.","Accommodation","Safety / LSA / FFA","Equipment Related","","","","","Sensors are already in order through SSUN23003-Last testing of alarms were satisfactory, No alarm on panel.","2023-09-14T23:59:35","SSUN230003","Completed","2023-09-14T23:59:35","No","No","No","Internal"]
[null,null,null,28360,22456,"55_Mon Jan 16 2023 06:07:58 GMT+0800","2022-12-14T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Walkway Fwd of midship not marked.","Miscellaneous","General Appearance","Inappropriate Procedure","11.8","Low","","","Painting Completed","2023-06-26T23:59:35","","Completed","2023-06-12T23:59:35","No","No","No","Internal"]
[null,null,null,28140,71489,"55_Wed Dec 28 2022 23:42:48 GMT+0800","2022-12-14T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","SOLAS TRAINING MANUALS was not made per ship Specific.","LSA / FFA","Safety / LSA / FFA","Human Error","5.15","Medium","","","* SOLAS TRAINING MANUALS to be made ship – Completed","2023-01-03T23:59:35","","Completed","2023-01-02T23:59:35","No","No","No","Internal"]
[null,null,null,28144,61013,"55_Wed Dec 28 2022 23:23:25 GMT+0800","2022-12-14T23:59:35","Observation","Owner / Marine / Tech. Suptd.","ISM Audit","Boiler in Pantry was not secured.","Accommodation","MLC Related","Human Error","11.13","Low","","","Boiler in Pantry secured with fixed securing arrangement.","2022-12-19T23:59:35","","Completed","2022-12-16T23:59:35","No","No","No","Internal"]
[null,null,null,28145,47746,"55_Wed Dec 28 2022 23:20:33 GMT+0800","2022-12-14T23:59:35","Observation","Owner / Marine / Tech. Suptd.","MLC Audit","Deep Fat Fryer in Galley was not secured.\n","Accommodation","MLC Related","Human Error","11.13","Low","","","Deep Fat Fryer in Galley secured With fixed securing arrangement..","2022-12-19T23:59:35","","Completed","2022-12-16T23:59:35","No","No","No","Internal"]
[null,null,null,28135,95809,"55_Wed Dec 28 2022 21:57:23 GMT+0800","2022-12-16T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Immersion Suit Air Pressure testing last carried out in Nov 2020, Manufactured in 2011. Annual pressure test required. Last Annual Carried out in Feb 2022 does not have records of Air Pressure test.","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.33","High","","","Immersion suits  Air Pressure tested using pressure testing kit available onboard.","2023-01-03T23:59:35","","Completed","2022-12-26T23:59:35","No","No","No","Internal"]
[null,null,null,29388,32838,"55_Thu Mar 16 2023 00:09:59 GMT+0800","2022-12-27T23:59:35","Observation,Non Conformity","Ship Staff","Nav Audit / Verification","During Navigational Audit found that Damage Control Plan was found missing from Emergency Plan Box on Bridge.","Navigation - Others","Navigation","Human Error","","","","","Same has been found in Bridge drawer and put back in place (Emergency Plan Box).","2023-03-26T23:59:35","","Completed","2022-12-27T23:59:35","No","No","No","Internal","Please discuss this observation and preventive action in next safety meeting/tool box meeting, with the officers/crew involved, to avoid recurrence."]
[null,null,null,28656,13559,"55_Sat Jan 21 2023 05:33:21 GMT+0800","2023-01-07T23:59:35","Defect","Ship Staff","Ship Staff Insp.","VECS o2 sensor is expired","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","","","","","Expired O2 sensor replaced with new one received and calibration carried out, working satisfactory.","2023-04-10T23:59:35","SSUN230044","Completed","2023-04-19T23:59:35","No","No","No","Internal"]
[null,null,null,28657,30947,"0_Sat Jan 21 2023 05:34:55 GMT+0800","2023-01-10T23:59:35","Defect","Ship Staff","Ship Staff Insp.","General service air line, valves are leaking and same needs to be attended.","Deck - Pipe / Fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Leaking air valves replaced.","2023-05-25T23:59:35","","Completed","2023-05-07T23:59:35","No","No","No","Internal"]
[null,null,null,28658,99965,"0_Sat Jan 21 2023 05:36:08 GMT+0800","2023-01-10T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Bunker manifold valves not holding same needs to be replaced.","Deck - Pipe / Fittings","MARPOL Related","Equipment Related","","","","","FO Bunker manifold valves (In total 4) replaced with new.  Line pressure tested at 4.4 bar. ","2023-08-30T23:59:35","","Completed","2023-08-29T23:59:35","No","No","No","Internal"]
[null,null,null,28659,63381,"55_Sat Jan 21 2023 05:57:16 GMT+0800","2023-01-10T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Funnel damper valve cylinder and air valves found to be leaking","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Spares received and new air cylinder fitted, tested , working satisfactorily.","2023-07-28T23:59:35","SSUN230054","Completed","2023-07-18T23:59:35","No","No","No","Internal"]
[null,null,null,28660,59151,"55_Tue Jan 31 2023 23:30:48 GMT+0800","2023-01-19T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","Main Air Compressor No. 2 breakdown due to loose securing screw of gudgeon pin causing gudgeon pin to move causing damage.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Overhaul of compressor with used spares to keep it standby for emergency use. Vessel raised requisition for spares. There is no running issues with MAC at present, Since Main Air compressor No.2 has been running last 6 months-with vessel monitoring continuously with Vibration readings -defect closed.","2023-09-29T23:59:35","SSUN230033, SSUN230066 & SSUN230090","Completed","2023-09-27T23:59:35","No","No","No","Internal"]
[null,null,null,28858,95098,"55_Wed Feb 15 2023 08:57:00 GMT+0800","2023-01-28T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Elevator inverter faulty and same needs to be replaced","Elect. Mach. & Equip.","","Equipment Related","","","","","Elevator inverter supplied, service engineer attended and same rectified","2023-02-19T23:59:35","ssun235007","Completed","2023-02-02T23:59:35","No","No","No","Internal"]
[null,null,null,28857,49227,"0_Wed Feb 15 2023 08:58:58 GMT+0800","2023-02-03T23:59:35","Defect","Ship Staff","Ship Staff Insp.","HFO Transfer pump coupling broken","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","","","","","transfer pump coupling renewed, pump tried out working satisfactory.","2023-06-11T23:59:35","SSUN230079","Completed","2023-06-06T23:59:35","No","No","No","Internal"]
[null,null,null,29370,41620,"55_Mon Mar 13 2023 11:19:22 GMT+0800","2023-02-13T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","SCBA compressor is used to charge both SCBA bottles and Lifeboat air bottles. \nSafety valve setting of 225 bar is for the safety of SCBA bottles. Does the vessel have separate safety valve when we are filling Lifeboat air bottle","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.43","High","","","Safety relief valve received","2023-07-13T23:59:35","","Completed","2023-07-02T23:59:35","No","No","No","Internal","This is a regulatory and a major safety issue and sooner or later will be pointed out during an external inspection. Please send us a separate mail and we will discuss this with the makers and advise the vessel to raise a new RO."]
[null,null,null,29374,69073,"55_Mon Mar 13 2023 11:12:48 GMT+0800","2023-02-13T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Crew members found drying up the clothes in the accommodation alley way","Accommodation","MLC Related","Behaviour Based","","","","","All clothes removed and crew members instructed not to dry clothes in alleyway. \nDedicated dry room and dryer to be used for the purpose. ","2023-03-07T23:59:35","","Completed","2023-02-21T23:59:35","No","No","No","Internal"]
[null,null,null,29375,84855,"55_Mon Mar 13 2023 11:25:17 GMT+0800","2023-02-13T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Receptacle for sound-powered telephone - cable insulation found damaged.","Miscellaneous","Communication","Equipment Related","","","","","Damaged Cable repaired. ","2023-03-23T23:59:35","","Completed","2023-02-22T23:59:35","No","No","No","Internal"]
[null,null,null,29376,86753,"55_Mon Mar 13 2023 11:32:29 GMT+0800","2023-02-13T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ER overhead crane hook secured with nylon slings. Change this to manila rope. ","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Human Error","","","","","Nylon Sling replaced with Manila Rope.","2023-03-23T23:59:35","","Completed","2023-02-22T23:59:35","No","No","No","Internal"]
[null,null,null,29377,82730,"55_Mon Mar 13 2023 11:36:30 GMT+0800","2023-02-13T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","5K250 valve in the ER found kept directly on the floor. To be kept on wooden plank","Miscellaneous","Eng. / Strg. Comp.","Human Error","","","","","Valve placed on wooden plank and secured. ","2023-03-23T23:59:35","","Completed","2023-02-24T23:59:35","No","No","No","Internal"]
[null,null,null,29378,23657,"55_Mon Mar 13 2023 11:39:17 GMT+0800","2023-02-13T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ME LOPx and FOPx feed temperature maintaining at 80-82 degC. \nTemperature to be maintained between 95-98 degC","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","","2023-03-23T23:59:35","","Completed","2023-02-26T23:59:35","No","No","No","Internal"]
[null,null,null,29379,17445,"55_Mon Mar 13 2023 11:44:41 GMT+0800","2023-02-13T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","24 alarms were in Off scanned condition during the visit. ","Miscellaneous","Eng. / Strg. Comp.","Behaviour Based","","","","","Same were removed from off scan during the visit. ","2023-03-23T23:59:35","","Completed","2023-02-13T23:59:35","No","No","No","Internal","Same were removed from off scan during the visit. "]
[null,null,null,29380,42136,"55_Mon Mar 13 2023 11:46:59 GMT+0800","2023-02-13T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Overwriting and corrections in the Engine  Log book were not counter signed by the Duty engineer","Documentation","Eng. / Strg. Comp.","Behaviour Based","","","","","All Overwriting and corrections in the Engine  Log book by Duty Engineer ","2023-03-23T23:59:35","","Completed","2023-02-22T23:59:35","No","No","No","Internal"]
[null,null,null,29381,79771,"55_Mon Mar 13 2023 11:49:33 GMT+0800","2023-02-13T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Wash basin in the ER found in very dirty condition","Miscellaneous","Eng. / Strg. Comp.","Behaviour Based","","","","","Wash Basin Cleaned.","2023-03-23T23:59:35","","Completed","2023-02-22T23:59:35","No","No","No","Internal"]
[null,null,null,29382,26724,"55_Mon Mar 13 2023 11:51:39 GMT+0800","2023-02-13T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Main Engine TC manometer to be filled with water","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","TC manometer filled with water","2023-03-23T23:59:35","","Completed","2023-02-24T23:59:35","No","No","No","Internal"]
[null,null,null,29383,28565,"55_Mon Mar 13 2023 11:53:50 GMT+0800","2023-02-13T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Few Quick closing valves in the ER found in very dirty condition. To be cleaned","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Quick closing valves cleaned.","2023-03-23T23:59:35","","Completed","2023-02-22T23:59:35","No","No","No","Internal"]
[null,null,null,29384,77014,"55_Mon Mar 13 2023 12:19:23 GMT+0800","2023-02-13T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","COP grease pots need to be filled up","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","","","","","COP grease pots filled up","2023-03-23T23:59:35","","Completed","2023-02-24T23:59:35","No","No","No","Internal"]
[null,null,null,29371,48420,"55_Tue Mar 14 2023 13:27:35 GMT+0800","2023-02-22T23:59:35","Defect","Ship Staff","Ship Staff Insp.","NO.1 AUX BOILER FD FAN BELLOW FOUND RUPTURED.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","AUX BOILER BELLOW REPLACED WITH SPARE NEW ONE","2023-07-17T23:59:35","","Completed","2023-07-17T23:59:35","No","No","No","Internal"]
[null,null,null,29373,27491,"55_Wed Mar 15 2023 23:19:43 GMT+0800","2023-02-25T23:59:35","Defect","Ship Staff","Ship Staff Insp.","HP DRUM GAUGE GLASS IS LEAKING.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Spare received, new gauge glass fitted.","2023-07-28T23:59:35","DSUN230029","Completed","2023-07-17T23:59:35","No","No","No","Internal"]
[null,null,null,29689,80798,"55_Sat Apr 01 2023 04:26:14 GMT+0800","2023-03-09T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Water mist repeater panel on bridge PCB burnt","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","",""," PCB unit received after repairs last call Singapore and tested, found working satisfactorily..(Repaired PCB fitted in ECR Repeater panel)","2023-07-13T23:59:35","SSUN230039","Completed","2023-07-13T23:59:35","No","No","No","Internal"]
[null,null,null,29690,86114,"0_Sat Apr 01 2023 04:28:03 GMT+0800","2023-03-19T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Various hydraulic fittings on staffa motor found to be rusted and same needs to be renewed.","Deck - Machinery,Deck - Mooring Machinery","Mooring","Equipment Related","9.14","Medium","","","Renewed leaky hydraulic fittings on mooring winch staffa motor.","2024-01-31T23:59:35","","Completed","2023-12-14T23:59:35","No","No","No","Internal","New fabricated spares have been supplied in Singapore and this job needs to be prioritized."]
[null,null,null,29968,68633,"55_Tue Apr 25 2023 22:01:14 GMT+0800","2023-03-24T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","RX-415, HC/O2 detector was found not giving “no pump suction” alarm. \nSimilarly, upon introducing calibration gas in normal mode there is no alarm activated when the O2 content falls. Also, the O2 reading does not go to zero on introducing 100% nitrogen. (Suspect internal leakage or faulty sensor)\n","Miscellaneous","Safety / LSA / FFA","Equipment Related","5.23","Very High","","","Received RX-415 along with rotation of Gas detectors. ","2023-06-24T23:59:35","SSUN235036","Completed","2023-07-02T23:59:35","No","No","No","Internal"]
[null,null,null,29974,61532,"55_Fri Apr 28 2023 05:06:26 GMT+0800","2023-04-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","NO.1 AUX BOILER IGNITION FLAME FAILURE TRIP AMPLIFIER IS NOT OPERATIONAL.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","TRIP AMPLIFIER CHANGED AND TRIED OUT WORKING SATISFACTORY.","2023-06-26T23:59:35","SSUN230085","Completed","2023-06-06T23:59:35","No","No","No","Internal"]
[null,null,null,29979,63213,"55_Mon May 01 2023 05:56:39 GMT+0800","2023-04-10T23:59:35","Defect","Ship Staff","Ship Staff Insp.","MAC 1  -Connecting rod bearing & Main bearing worn","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related","","","","","MAC I Complete overhaul -5000 hrs routine carried out, Bearings & Piston rings renewed.","2023-04-15T23:59:35","","Completed","2023-04-18T23:59:35","No","No","No","Internal"]
[null,null,null,29970,92219,"55_Tue Apr 25 2023 22:06:07 GMT+0800","2023-04-11T23:59:35","Observation","Ship Staff","Ship Staff Insp.","PORT LIFEBOAT ENTERANCE EMBARKATION RAILING FOUND TO HAVE CORRODED AND HAVING A HOLE   ","","Safety / LSA / FFA","Equipment Related","5.29","High","","","Lifeboat Access Door Railing, Top Railing removed found corroded \nNew railing fabricated. \nInstalled in location, Primer and final coat completed, covered with Tiger Strip Tape. ","2023-05-24T23:59:35","","Completed","2023-05-05T23:59:35","No","No","No","Internal"]
[null,null,null,29967,62460,"55_Tue Apr 25 2023 21:59:20 GMT+0800","2023-04-12T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Hoisting wire on port side ladder to sunken deck from upper deck, has only two turns on the drum","Deck - Machinery","Safety / LSA / FFA","Equipment Related","5.47","Medium","","","Port Side ISPS Ladder, heaved up during test and checks for transiting Malacca and Singapore straights found in working order.  \n ","2023-06-24T23:59:35","SSUN230121","Completed","2023-05-25T23:59:35","No","No","No","Internal"]
[null,null,null,29966,94549,"55_Tue Apr 25 2023 21:57:29 GMT+0800","2023-04-14T23:59:35","Observation","Ship Staff","Ship Staff Insp.","STBD WINDLASS, MOORING DRUMS AND FITTINGS JERKING DURING LOWERING/SLACKNING","Deck - Mooring Machinery","Mooring","Equipment Related","","","","","","2023-09-14T23:59:35","","Completed","2023-06-13T23:59:35","No","No","No","Internal"]
[null,null,null,30243,91461,"55_Tue May 16 2023 02:30:52 GMT+0800","2023-04-15T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Starboard Bridge Wing ME Control unit BWU09-Lever (Telegraph), pot meter faulty.","E/R - Main Engine","Navigation","Equipment Related","10.32","Very High","","","Starboard Bridge Wing ME Control unit LTU was replaced with spare one by Service engineer. Tested and found satisfactory. ","2023-11-29T23:59:35","","Completed","2023-11-23T23:59:35","No","No","No","Internal","Service attendance will be planned from Kongsberg from makers "]
[null,null,null,29971,10140,"55_Tue Apr 25 2023 22:07:24 GMT+0800","2023-04-16T23:59:35","Observation","Ship Staff","Ship Staff Insp.","TORCH FOR FIRE MAN OUTFITS, FOUND TO BE OF LESS INTENSITY. ","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.43","High","","","Replacement received and placed at designated locations. ","2023-06-24T23:59:35","SSUN230086","Completed","2023-06-06T23:59:35","No","No","No","Internal"]
[null,null,null,29972,83186,"55_Tue Apr 25 2023 22:08:12 GMT+0800","2023-04-16T23:59:35","Observation","Ship Staff","Ship Staff Insp.","GLOVES FOR FIREMAN OUTFITS (2 SETS) ARE SMALL SIZE, DOES NOT FIT TO MANY CREW MEMBERS.","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.43","High","","","Spares received and placed at designated locations. ","2023-06-24T23:59:35","SSUN230086","Completed","2023-06-06T23:59:35","No","No","No","Internal"]
[null,null,null,29973,17971,"55_Thu Apr 27 2023 18:03:34 GMT+0800","2023-04-16T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","Neil Robertson Stretcher in Pumproom, found with strap broken. ","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.20","Medium","","","Broken Strap Stitched, and stretcher put back in location. ","2023-05-26T23:59:35","","Completed","2023-04-27T23:59:35","No","No","No","Internal"]
[null,null,null,29978,77101,"55_Tue Apr 25 2023 22:03:25 GMT+0800","2023-04-16T23:59:35","Observation","Ship Staff","Ship Staff Insp.","BREATHER VALVE FOR INERT GAS LINE FOUND TO BE PASSING AT PRESSURE GREATER THAN 400 MMWG","Cargo Mach.","Safety / LSA / FFA","Equipment Related","8.41","Medium","","","breather valve removed from location, found to have pittings, same have been attended and boxed back. Once IG is Topped Up will monitor again for any signs of leaks. Presently no leak noticed till 400 mmwg. ","2023-06-24T23:59:35","","Completed","2023-04-22T23:59:35","No","No","No","Internal"]
[null,null,null,29976,83047,"55_Mon May 01 2023 07:14:23 GMT+0800","2023-04-17T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Unable to connect the Intrinsically Safe Camera provided for use on Deck to any of the Computers, including Master’s Computer.\nUpon connecting to any device “USB Device Not Recognized” Warning is flashed.\nDetails of the phone are \nModel Number: Impact X\nDevice Name: Impact X-PXIMEX14006225\nAndroid Version 5.1.1\nBluetooth transferring was tested, did not happen.\n","Miscellaneous","Safety / LSA / FFA","Equipment Related","5.6","Low","","","It is not getting connected with the supplied USB cable but it got connected by the crew’s USB cable. Same was tested on Ship’s Computer, and the phone got connected using crew’s USB cable. The supplied USB cable is only charging the device and is not supporting file transfer.  Requisition has been raised for same. \n","2023-07-17T23:59:35","SSUN230083","Completed","2023-05-13T23:59:35","No","No","No","Internal"]
[null,null,null,29969,20036,"55_Tue Apr 25 2023 22:02:29 GMT+0800","2023-04-18T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","JOINING ANGLE BETWEEN RAILINGS (NEAR OP 285) IN PUMPROOM ON STAIR CASE LEADING TO TRO UNIT PLATFORM FOUND BROKEN FROM ONE END.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","","","","","Bracket and Bolt Arrangement made and railings secured, \nPrimer and Final Coat Applied. ","2023-06-24T23:59:35","","Completed","2023-04-28T23:59:35","No","No","No","Internal"]
[null,null,null,29977,80031,"55_Mon May 01 2023 07:26:36 GMT+0800","2023-04-23T23:59:35","Defect","Ship Staff","Ship Staff Insp.","AFT ETA,  Towing Pennant Drum Found Seized and Unmovable during Routine Inspection and Drills","LSA / FFA","Safety / LSA / FFA","Equipment Related","9.28","Medium","","","Break had got seized due to rusting, same was dismantled and cleared of all corrosion. \nTested for operation, working satisfactory. ","2023-06-01T23:59:35","","Completed","2023-04-27T23:59:35","No","No","No","Internal"]
[null,null,null,30241,91988,"55_Thu May 11 2023 23:07:36 GMT+0800","2023-04-27T23:59:35","Defect","Ship Staff","Ship Staff Insp."," AUS pumps casing temperature gauges are not working.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.80","Medium","","","New spares received, installed and made operational.","2023-10-14T23:59:35","SSUN230102","Completed","2023-10-08T23:59:35","No","No","No","Internal"]
[null,null,null,30244,99906,"55_Thu May 11 2023 23:11:23 GMT+0800","2023-04-27T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Steering Gear Walkway Gratings are not secured","Miscellaneous","Eng. / Strg. Comp.","Inappropriate Procedure","10.43","Medium","","","Steering gear room walkway gratings secured.","2023-05-26T23:59:35","","Completed","2023-05-14T23:59:35","No","No","No","Internal"]
[null,null,null,30242,95702,"55_Fri May 12 2023 19:07:48 GMT+0800","2023-04-29T23:59:35","Defect","Ship Staff","Ship Staff Insp.","IG AND IGG SCRUBBER OVBD VALVES REMOTE OPERATION INDICATION JUNCTION BOX ES AT SUNKEN DECK ARE COMPLETELY WASTED.","Elect. Mach. & Equip.","General Appearance","Equipment Related","10.37","Medium","","","All junction boxes were covered by a separate metal cover to cover the complete valve along with the junction boxes, All cable connections were properly secured.","2023-07-28T23:59:35","","Completed","2023-07-19T23:59:35","No","No","No","Internal"]
[null,null,null,30345,96871,"55_Fri Jun 02 2023 15:34:00 GMT+0800","2023-05-12T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Main engine no.1 unit exhaust valve stroke sensor is faulty.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","storke sensor replaced with new one after stopping main engine, now working satisfactory.","2023-05-27T23:59:35","","Completed","2023-05-22T23:59:35","No","No","No","Internal"]
[null,null,null,30342,35263,"55_Fri Jun 02 2023 08:45:58 GMT+0800","2023-05-28T23:59:35","Observation","Ship Staff","Ship Staff Insp.","BWTS TRO Detection Cabinets AIT-151 & AIT-251, should show Green Light for Pressure, Timer & By-Pass at all times. The Light for Pressure and By-Pass are turning to Red after some interval. Suspect leak of Positive Pressure or insufficient positive pressure. ","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.13","Medium","","","Another Thin Gasket has been placed underneath the Original Gasket inside the Cabinet Door, to increase the area of contact. \nPresently all 3 lights are showing green. ","2023-06-26T23:59:35","","Completed","2023-06-06T23:59:35","No","No","No","Internal"]
[null,null,null,30344,33052,"55_Fri Jun 02 2023 20:47:03 GMT+0800","2023-05-29T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Minor seepage noticed in VRCS Return Line under U Clamp, in vicinity of Foam Monitor # 7","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.11","Medium","","","Section cropped and replaced. \nPut back in location and system tested, found in order. ","2023-06-26T23:59:35","","Completed","2023-05-30T23:59:35","No","No","No","Internal"]
[null,null,null,30499,47217,"55_Tue Jun 13 2023 17:29:04 GMT+0800","2023-05-30T23:59:35","Defect","Ship Staff","Ship Staff Insp.","AFT HYDRAULIC MACHINERY ALARMS ARE NOT CONNECTED TO AMS PANEL.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","FAULT RECTIFIED AND ALARM TESTED, WORKING SATISFACTORY","2023-07-16T23:59:35","","Completed","2023-08-07T23:59:35","No","No","No","Internal"]
[null,null,null,30500,46875,"55_Thu Jun 15 2023 15:29:29 GMT+0800","2023-06-02T23:59:35","Defect","Ship Staff","Ship Staff Insp.","No.1 FWG Ejector pump discharge valve to the EGB washing line is having a pinhole.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.31","Very High","","","Vessel changed the FWG ejector pump No. 1 discharge valve to WHRS wash water line with new spare. Valve tested while water washing WHRS.","2023-10-29T23:59:35","SSUN230185","Completed","2023-10-11T23:59:35","No","No","No","Internal"]
[null,null,null,30502,60315,"55_Thu Jun 15 2023 15:33:07 GMT+0800","2023-06-03T23:59:35","Defect","Ship Staff","Ship Staff Insp.","EGB drain valve is not holding smoke is leaking to soot tank","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.31","Very High","","","EGB drain valve to soot tank replaced with new, which was received during vessels last call at Singapore.","2023-08-09T23:59:35","","Completed","2023-08-03T23:59:35","No","No","No","Internal"]
[null,null,null,30948,23198,"55_Sat Jul 01 2023 09:24:55 GMT+0800","2023-06-23T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Ship Staff Insp.","AUX ENGINE AIR SCAVENGE MANIFOLD DRAIN LINES TO BE SEPRATED FROM DRAIN BOX AND FITTED INDIVIDUALLY WITH  3MM ORIFICE.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","ALL DRAIN LINES SEPARATED , BALL VALVE  INSTALLED KEPT OPEN -REGULATED TO MONITOR DRAINS ARE CLEAR.","2023-07-29T23:59:35","","Completed","2023-07-11T23:59:35","No","No","No","Internal"]
[null,null,null,30943,75923,"55_Sat Jul 15 2023 23:14:36 GMT+0800","2023-07-02T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Fwd and after hydraulic motor for deck power pack, does not have any inspection hole for inspection of coupling. \t\t","Deck - Machinery","Mooring","Equipment Related","","","","","Hole Made as instructed.","2023-08-09T23:59:35","","Completed","2023-08-01T23:59:35","No","No","No","Internal"]
[null,null,null,30944,58604,"55_Sat Jul 15 2023 23:16:31 GMT+0800","2023-07-02T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","On main deck Walkway stanchion wire in corroded condition\t\t","Miscellaneous","Safety / LSA / FFA","Equipment Related","","","","","Wires de rusted and greased. ","2023-08-29T23:59:35","","Completed","2023-07-23T23:59:35","No","No","No","Internal"]
[null,null,null,30945,96170,"55_Sun Jul 16 2023 03:27:38 GMT+0800","2023-07-02T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Engine room Blower casing to de-rust and paint","Miscellaneous","General Appearance","Equipment Related","","","","","Blower casing  de-rusted and painted","2023-10-02T23:59:35","","Completed","2023-09-17T23:59:35","No","No","No","Internal","Maintenance to be prioritized "]
[null,null,null,30946,62384,"55_Sun Jul 16 2023 03:30:43 GMT+0800","2023-07-02T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Engine Casing Funnel spot rust to touch up","Deck - Pipe / Fittings","General Appearance","Equipment Related","","","","","Funnel Casing Forward, Port and Stbd side bulkhead spot de-rusted, primer and final coat completed.","2023-08-13T23:59:35","","Completed","2023-08-07T23:59:35","No","No","No","Internal"]
[null,null,null,30947,23839,"55_Sat Jul 15 2023 23:18:00 GMT+0800","2023-07-02T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Water collected in the stripping pump save all. TO find the source of leak and rectify","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","Water was drained during the Warming Up procedure of the stripper pump as vessel had used stripper pump for de slopping at Singapore on 04 Aug 23. \nAll water from drip tray has been removed and cleaned.  ","2023-07-20T23:59:35","","Completed","2023-07-06T23:59:35","No","No","No","Internal"]
[null,null,null,31687,38450,"55_Tue Aug 22 2023 01:51:57 GMT+0800","2023-07-31T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Gear Oil Dripping Leak noticed on Port Side Windlass, from underneath the shaft in between the Windlass and the Inboard mooring rope drum.   ","Deck - Machinery","Mooring","Equipment Related","9.20","Medium","","","Breather valve found seized same pressurising gear case, same eased up. Oil level maintained in the sight glass. Operation checked and no leaks observed.","2023-12-31T23:59:35","","Completed","2023-10-27T23:59:35","No","No","No","Internal"]
[null,null,null,31691,56801,"55_Tue Aug 22 2023 01:42:52 GMT+0800","2023-08-07T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","Aft Mooring Winch Motor - Return Line For Hydraulic Oil, Soft Patch Formation and Leaking. \n","Deck - Pipe / Fittings","Mooring","Equipment Related","11.4","Very High","","","Permanent repaired carried out, by crop and renew the stub piece.Hydraulic return line tested after repair, found in order.\n","2023-11-29T23:59:35","","Completed","2023-11-18T23:59:35","No","No","No","Internal"]
[null,null,null,31688,95600,"55_Sat Aug 26 2023 02:49:59 GMT+0800","2023-08-12T23:59:35","Defect","Ship Staff","Ship Staff Insp.","BWTS Neutralization pump discharge line going to pump room has several leaks in engine room. Leaks are due to material failure of the discharge tubing.","E/R - Pipes/ valves & fittings","Cargo / Ballast Systems","Equipment Related","","","","","All lines renewed with new material supplied. Line pressure tested after repair and found in good order.","2023-10-29T23:59:35","SSUN230164 (Received onboard)","Completed","2023-10-26T23:59:35","No","No","No","Internal"]
[null,null,null,31689,22721,"55_Wed Aug 30 2023 08:11:02 GMT+0800","2023-08-25T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Water Ballast Tank Fixed Gas Detection System Giving Internal Leakage Alarm Repeatedly ","Deck - Machinery","Cargo / Ballast Systems","Equipment Related","","","","","Both sampling pump diaghram renewed and system made operational without any alarm.","2023-10-29T23:59:35","","Completed","2023-09-07T23:59:35","No","No","No","Internal"]
[null,null,null,31903,30930,"55_Thu Sep 14 2023 17:43:54 GMT+0800","2023-09-02T23:59:35","Defect","Ship Staff","Ship Staff Insp.","ME No.1 Unit Cylinder cover crack confirmed from leak through Star air pipe pocket-finding its way to Start air manifold","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.10","High","","","Replaced cylinder cover for Unit No.1 ","2023-09-04T23:59:35","","Completed","2023-09-03T23:59:35","No","No","No","Internal"]
[null,null,null,31902,57113,"55_Fri Sep 15 2023 09:59:17 GMT+0800","2023-09-03T23:59:35","Defect,Non Conformity","Ship Staff","Ship Staff Insp.","ME No.1 Unit Liner Jacket l(Lower) has a crack.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","ME unit Cylinder liner removed and new Lower Liner water jacket installed. Job carried out by Shore Workshop at Singapore","2023-09-11T23:59:35","","Completed","2023-09-11T23:59:35","No","No","No","Internal"]
[null,null,null,31893,94141,"55_Thu Sep 14 2023 11:39:02 GMT+0800","2023-09-10T23:59:35","Defect","Ship Staff","Ship Staff Insp.","VECS Oxygen Sensor at Manifold not giving correct reading of Oxygen Level ","Inert Gas","Safety / LSA / FFA","Equipment Related","8.17","Low","","","All sampling lines, unions, and flowmeter cleared as same were blocked with carbon deposits. Damaged sampling lines renewed. Sensor calibrated and system observed for 3 days. System found to be operating normal.\n","2023-10-30T23:59:35","","Completed","2023-10-29T23:59:35","No","No","No","Internal"]
[null,null,null,31901,94074,"55_Fri Sep 29 2023 00:08:23 GMT+0800","2023-09-11T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","Engine room crane High Hoist motor not working-Motor shaft spline sheared off","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","New hoisting motor along with brake assembly installed. Engine room crane load tested and put in service.","2023-10-04T23:59:35","SSUN 230190 & SSUN230040","Completed","2023-10-04T23:59:35","No","No","No","Internal"]
[null,null,null,31896,68681,"55_Fri Sep 29 2023 00:32:17 GMT+0800","2023-09-23T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Overboard pipe of EGCS-GRP near AE's -pipe flange to have splash-Guards around -to avoid water splash on AE's .","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.23","Medium","","","Fabrication and installation of guard cover for GRP Pipe flanges using GI Sheets is complete. All flanges of EGCS overboard pipe near auxiliary engines have anti-splash protection cover.","2023-11-29T23:59:35","","Completed","2023-10-27T23:59:35","No","No","No","Internal"]
[null,null,null,31899,64187,"55_Fri Sep 29 2023 00:50:10 GMT+0800","2023-09-23T23:59:35","Defect,Observation","Ship Staff","Ship Staff Insp.","The drains for Funnel deck save all drain line are  choked and the water does not drain from the save all-as a result the water splashes on to the electrical Lamp fitting.(Near Port side ER Blower)","Deck - Pipe / Fittings","General Appearance","Equipment Related","","","","","Drains cleared.","2023-10-29T23:59:35","","Completed","2023-10-26T23:59:35","No","No","No","Internal"]
[null,null,null,32858,99712,"55_Tue Oct 31 2023 10:04:10 GMT+0800","2023-10-17T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","NO. 1 Air condition compressor controller unit found with no power / display. Main PCB was defective.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.30","High","","","AC controller unit (Type ACS 2) replaced with new spare. Unit programmed and put in service.","2023-10-31T23:59:35","","Completed","2023-10-24T23:59:35","No","No","No","Internal"]
[null,null,null,32857,91244,"55_Mon Oct 30 2023 20:28:17 GMT+0800","2023-10-21T23:59:35","Defect","Ship Staff","Ship Staff Insp.","STBD crane block sheeve is in ceased condition.","Deck - Machinery","Safety / LSA / FFA","Equipment Related","8.50","Medium","","","STBD crane block sheeves removed from crane block. De rusting, painting freeing up carried out on the same and put back in position. ","2023-10-31T23:59:35","","Completed","2023-10-26T23:59:35","No","No","No","Internal"]
[null,null,null,32856,62737,"55_Mon Oct 30 2023 20:17:44 GMT+0800","2023-10-22T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Both port and stbd gangway sheeves are in rusted condition.","Deck - Pipe / Fittings","Safety / LSA / FFA","Equipment Related","5.47","Medium","","","Port and stbd accommodation ladder sheeves removed. Freeing up, de rusting and painting, greasing carried out on same and put back in position.  ","2023-10-30T23:59:35","","Completed","2023-10-28T23:59:35","No","No","No","Internal"]
[null,null,null,32861,45728,"55_Tue Oct 31 2023 16:45:48 GMT+0800","2023-10-28T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Foam monitor no.7 valve is in ceased condition.","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.38","High","","","Overhauling / freeing up of no7 foam isolation valve carried out, Pressure testing of same done, found in order.\n","2023-11-02T23:59:35","","Completed","2023-11-01T23:59:35","No","No","No","Internal"]
[null,null,null,32859,80019,"55_Tue Oct 31 2023 10:12:27 GMT+0800","2023-10-30T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","HFO purifier No. 2 motor found making abnormal noise. Motor insulation recorded as 0.5 Mega-ohms.   ","E/R - Purifier","Eng. / Strg. Comp.","Equipment Related","10.3","Medium","","","Vessel installed one spare motor of same model with 22 Kw rating (Original motor with 26 Kw rating),  New contactor received and installed for starting panel. Purifier tried out and found working satisfactory.","2023-11-30T23:59:35","SSUN230208 - El. Motor\nSSUN230211 - Magnetic contactor for starter panel","Completed","2023-11-21T23:59:35","No","No","No","Internal"]
[null,null,null,32852,47931,"55_Wed Nov 08 2023 10:24:44 GMT+0800","2023-11-08T23:59:35","Other","Ship Staff","Ship Staff Insp.","Vessel is fitted with Fixed CO2 fire extinguishing system for machinery space, pump room & emergency generator room, manufactured by NK Co. LTD. The manufacturing date for the system is 01-NOV-2011. Vessel received Marine safety advisory notice No. 14 of 2023, which states, \"change of material of bursting disc on carbon dioxide cylinder valves from copper to nickel\". The cylinder valve will have to be changed to renew bursting disc. ","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","Cylinder valves for individual carbon dioxide cylinders will have to be changed to renew bursting disc. The job has been shifted to REFMAN.","2027-01-01T23:59:35","","Completed","2023-12-05T23:59:35","No","No","No","Internal"]
[null,null,null,32860,69330,"55_Thu Nov 30 2023 20:28:28 GMT+0800","2023-11-28T23:59:35","Defect","Ship Staff","Ship Staff Insp.","No.3 STBD side window wiper was not operational. ","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","On investigation, found belt broken. Same replaced with spare new belt. Tested and working satisfactory. ","2023-11-30T23:59:35","","Completed","2023-11-30T23:59:35","No","No","No","Internal"]
[null,null,null,33323,77696,"55_Fri Dec 15 2023 16:01:01 GMT+0800","2023-12-07T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Running hour meter for Service air compressor was in-operational. ","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related","10.3","Medium","","","Running hour meter for Service air compressor was replaced with spare new one. ","2023-12-13T23:59:35","","Completed","2023-12-08T23:59:35","No","No","No","Internal"]
[null,null,null,33320,14858,"55_Fri Dec 15 2023 15:34:45 GMT+0800","2023-12-08T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Port side Hose handling crane heaving limit was rusted but operational. ","Deck - Machinery","Cargo / Ballast Systems","Equipment Related","9.20","Medium","","","The limit switch was replaced with spare new one and the rusted one cleaned and  lubricated.  ","2023-12-08T23:59:35","","Completed","2023-12-08T23:59:35","No","No","No","Internal"]
[null,null,null,33322,21713,"0_Fri Dec 15 2023 15:48:18 GMT+0800","2023-12-11T23:59:35","Defect","Ship Staff","Ship Staff Insp.","While carrying out the calibration of the inlet water analyser of the EGCS System, found the drain pipe of the scupper obstructing the placement of the portable display unit of EGCS. ","E/R - Aux. Mach.","Eng. / Strg. Comp.","External Factors","10.30","High","","","The drain pipe above the inlet analyser was removed and modified and fitted back. ","2023-12-16T23:59:35","","Completed","2023-12-15T23:59:35","No","No","No","Internal"]
[null,null,null,33321,48224,"0_Fri Dec 15 2023 15:38:18 GMT+0800","2023-12-12T23:59:35","Defect","Ship Staff","Ship Staff Insp.","When trying out AE LO purifier, found lube oil leaking from end flange of the heater. ","E/R - Purifier","Eng. / Strg. Comp.","Equipment Related","10.30","High","","","Purifier was stopped. Heater drained and the element was removed from place. Gaskets renewed and system tried out and found no leaks. ","2023-12-14T23:59:35","","Completed","2023-12-13T23:59:35","No","No","No","Internal"]
[null,null,null,33324,13889,"55_Fri Dec 15 2023 15:58:30 GMT+0800","2023-12-15T23:59:35","Defect","Ship Staff","Ship Staff Insp.","During routine inspection, Steering gear room phone cord was found to be brittle. ","Elect. Mach. & Equip.","Eng. / Strg. Comp.","External Factors","11.10","Medium","","","Phone cord was replaced with spare new one. ","2023-12-15T23:59:35","","Completed","2023-12-15T23:59:35","No","No","No","Internal"]
[null,null,null,null,16437,"55_Mon Jan 08 2024 16:08:41 GMT+0800","2024-01-05T08:00:00","Defect","Ship Staff","Ship Staff Insp.","NO.2 DG Unit No.5 Main Bearing temperature reading found to be erractic and giving alarm","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.30","High","","","Stopped the DG and found the temperature sensor to be defective. Replaced with spare one onboard and DG started. All found satisfactory. ","2024-01-05T08:00:00","","Completed","2024-01-05T08:00:00","No","No","No","Internal"]
[null,null,null,null,94311,"55_Fri Sep 29 2023 00:36:21 GMT+0800","2023-09-26T08:00:00","Defect","Ship Staff","Ship Staff Insp.","EGCS Effluent flow sensor defective -PCB Burnt","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.11","Medium","","","New EGCS Effluent flow sensor received in Singapore transit and was changed. Now, its operational. ","2024-01-31T08:00:00","SSUN230193","Completed","2024-01-05T08:00:00","No","No","No","Internal"]
[null,null,null,null,29484,"55_Wed Jun 15 2022 02:36:41 GMT+0800","2022-11-15T08:00:00","Defect","Ship Staff","Ship Staff Insp.","CLO pump worn off alarm is appearing while running ICO lube.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Both Stator of System oil and cylinder oil pump renewed with spare received. System tried out and all found satisfactory. \n","2024-01-31T08:00:00","SSUN230009","Completed","2023-12-14T08:00:00","No","No","No","Internal",""]
[null,null,null,null,69891,"55_Wed Mar 15 2023 16:36:07 GMT+0800","2023-02-13T08:00:00","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Starboard void space local gauge cable found damaged","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Spares received and changed the content guage. All found satisfactory. ","2024-01-31T08:00:00","SSUN230078","Completed","2024-01-24T08:00:00","No","No","No","Internal"]
[null,null,null,null,75636,"55_Mon Jun 12 2023 15:58:04 GMT+0800","2023-05-30T08:00:00","Defect","Ship Staff","Ship Staff Insp.","OILY WATER SEPERATOR FLOW SWITCH OPERATION IS ERRATIC.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Spare received and replaced with new one. ","2024-01-31T08:00:00","SSUN230124","Completed","2024-01-24T08:00:00","No","No","No","Internal"]
[null,null,null,null,68226,"55_Fri Feb 02 2024 11:22:25 GMT+0800","2024-01-27T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Pressure gauges of Aft Hydraulic pump No.1 and No.2 were defective. ","Deck - Mooring Machinery","Eng. / Strg. Comp.","Equipment Related","9.20","Medium","","","Replaced with pressure gauges with spare new one. ","2024-02-01T08:00:00","","Completed","2024-01-28T08:00:00","No","No","No","Internal"]
[null,null,null,null,66198,"55_Tue Oct 31 2023 09:51:57 GMT+0800","2023-10-21T08:00:00","Breakdown","Ship Staff","Ship Staff Insp.","HFO purifier No. 2 pneumatically operated 3-way valve malfunctioning. Operation of 3-way valve is erratic due to improper sealing of air piston & cylinder. ","E/R - Purifier","Eng. / Strg. Comp.","Equipment Related","10.3","Medium","","","Replaced the 3 way valve with new spare received. System tried out. All found satisfactory. ","2024-02-06T08:00:00","SSUN230203","Completed","2024-02-02T08:00:00","No","No","No","Internal","Spares will be arranged at Singapore in Jan 2024."]
[null,null,null,null,65451,"55_Thu Feb 15 2024 14:40:24 GMT+0800","2024-02-12T08:00:00","Defect","Ship Staff","Ship Staff Insp.","No.1 Economiser Feed Pump observed to be having vibration from the pump end. ","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","The Pump was opened up for inspection. On inspection, found the shaft bearing close to the motor coupling worn out and Intermediate sleeve missing. Same replaced with spare one onboard. All O rings, gaskets, packings and mechanical seal renewed. Pump tried out and found to be in working condition. ","2024-02-15T08:00:00","","Completed","2024-02-13T08:00:00","No","No","No","Internal"]
[null,null,null,null,55697,"55_Thu Feb 15 2024 14:43:49 GMT+0800","2024-02-09T08:00:00","Defect","Ship Staff","Ship Staff Insp.","No.1 HFO purifier supply pump magnectic coupling cover housing damaged. ","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","No.1 HFO purifier supply pump opened up and on inspection found the bearing damaged. Same replaced with new spare one. Pump rotor magnectic coupling replaced as it was damaged too. All gaskets and O rings changed. Pump tried out. All found satisfactory. ","2024-02-10T08:00:00","","Completed","2024-02-10T08:00:00","No","No","No","Internal"]
[null,null,null,null,56552,"55_Fri Oct 20 2023 14:50:03 GMT+0800","2023-07-13T08:00:00","Defect","Ship Staff","Ship Staff Insp.","VRCS system main line pressure relief valve is leaking, causing frequent loading/unloading of unloader for running pump and frequent cut in/cut off of stand by pump.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.30","High","","","Replaced the relief valve and system tried out. System is operational and tried out during one loading and discharging operation.","2024-02-29T08:00:00","DSUN230153","Completed","2024-02-22T08:00:00","No","No","No","Internal"]
[null,null,null,null,65187,"55_Fri Feb 02 2024 13:08:38 GMT+0800","2024-01-24T08:00:00","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Numerous breather valves on mooring winches have been found painted and ring missing to pull out the breather valve.","Deck - Mooring Machinery","Mooring","Equipment Related","9.14","Medium","","","Breather valve on all mooring winches free from paint and in working order. RIngs fitted as applicable ","2024-02-24T08:00:00","","Completed","2024-02-29T08:00:00","No","No","No","Internal"]
[null,null,null,null,86414,"55_Fri Mar 01 2024 20:33:25 GMT+0800","2024-02-22T08:00:00","Observation","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","The two horizontal motor shafts of the AUS vacuum pump unit installed on the second deck at the top of the pump room were not completely provided with safety guards, and the each rotary shaft was approximately 35cm exposed.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","5.11","Low","",""," Protection covers have been fabricated on board and installed to completely shield the exposed shaft sections of both the horizontal motor shafts of the AUS vacuum pump units.\nAll other pump shafts were checked onboard and found to be adequately covered with safety guards.\n\n\n","2024-03-22T08:00:00","","Completed","2024-02-26T08:00:00","No","No","No","External"]
[null,null,null,null,84084,"55_Fri Mar 01 2024 20:37:08 GMT+0800","2024-02-22T08:00:00","Observation","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","Low air pressure alarming device (whistle type) of a SCBA set located in the fire control station was defective and not activated alarming sound when tested. (The whistling device of the SCBA was loose and removing easily, if fixed it firmly then not activating alarming sound when tested.)","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.43","High","","","We wish to confirm that the SCBA Set whistle was aligned correctly and the Allen bolt adequately tightened during the inspection and the same rectified prior inspector’s disembarkation. The SCBA set whistle was tested multiple times and found to be in good working order. \n\nAll other SCBA set whistles and other components were checked for tightness and found to be in order.\n","2024-03-22T08:00:00","","Completed","2024-02-26T08:00:00","No","No","No","External"]

{"sheet":"Calc","index":2,"n_rows":28,"n_cols":12,"rows_kept":28,"cut":false,"hidden":true,"merged":[]}
["Def_type","Def_cause","Equipments","VIQrefno","Observer_code"]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,"Dim itemSele As Long"]
[null,null,null,null,null,null,null,null,null,null,null,"   dim startRow as integer"]
[null,null,null,null,null,null,null,null,null,null,null,"   startRow=1"]
[null,null,null,null,null,null,null,null,null,null,null,"        For itemSele = 0 To ListBox1.ListCount - 1"]
[null,null,null,null,null,null,null,null,null,null,null,"        If ListBox1.Selected(itemSele) = True Then"]
[null,null,null,null,null,null,null,null,null,null,null,"        Worksheets(\"WorksheetName\").Range(\"A\" & startRow).Value = ListBox1.List(itemSele)"]
[null,null,null,null,null,null,null,null,null,null,null,"        startRow = startRow + 1"]
[null,null,null,null,null,null,null,null,null,null,null,"        End If"]
[null,null,null,null,null,null,null,null,null,null,null,"        Next"]
[null,null,null,null,null,null,null,null,null,null,null,"Dim LastRowA As String"]
[null,null,null,null,null,null,null,null,null,null,null,"        Dim itemSele As Long"]
[null,null,null,null,null,null,null,null,null,null,null,"       Dim startRow as integer"]
[null,null,null,null,null,null,null,null,null,null,null,"        LastRowA = ActiveSheet.Cells(Rows.count, \"A\").End(xlUp).row"]
[null,null,null,null,null,null,null,null,null,null,null,"        startQue = 0"]
[null,null,null,null,null,null,null,null,null,null,null,"        For itemSele = 0 To ListBox1.ListCount - 1"]
[null,null,null,null,null,null,null,null,null,null,null,"        For startRow = 1 To LastRowA"]
[null,null,null,null,null,null,null,null,null,null,null,"        If Worksheets(\"WorksheetName\").Range(\"A\" & startRow).Value = ListBox1.List(itemSele) Then"]
[null,null,null,null,null,null,null,null,null,null,null,"        ListBox1.Selected(itemSele) = True"]
[null,null,null,null,null,null,null,null,null,null,null,"        Exit For"]
[null,null,null,null,null,null,null,null,null,null,null,"        End If"]
[null,null,null,null,null,null,null,null,null,null,null,"        Next j"]
[null,null,null,null,null,null,null,null,null,null,null,"        Next"]
[null,null,null,null,null,null,null,null,null,null,null,"        End If"]

{"sheet":"Areaofobs","index":3,"n_rows":17,"n_cols":2,"rows_kept":17,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Cargo / Ballast Systems",11]
["Cert. & Docu.",2]
["Communication",6]
["Crew Management",3]
["Emgcy. Systems",13]
["Eng. / Strg. Comp.",14]
["General Appearance",15]
["Ice Opns.",17]
["ISM Related",7]
["ISPS Related",10]
["MARPOL Related",9]
["MLC Related",4]
["Mooring",12]
["Navigation",5]
["Safety / LSA / FFA",8]
["Structural Condn. / WT integrity ",16]

{"sheet":"Vessel_type","index":4,"n_rows":1,"n_cols":2,"rows_kept":1,"cut":false,"hidden":true,"merged":[]}
["Vessel_type","ID"]

{"sheet":"Deficiency_type","index":5,"n_rows":8,"n_cols":3,"rows_kept":8,"cut":false,"hidden":true,"merged":[]}
["TITLE","Type of deficiency_description","ID"]
["Breakdown",null,6]
["Critical Equipment",null,4]
["Defect",null,1]
["Guarantee Claim",null,8]
["Non Conformity",null,2]
["Observation",null,3]
["Other",null,7]

{"sheet":"VIQrefno","index":6,"n_rows":427,"n_cols":3,"rows_kept":427,"cut":false,"hidden":true,"merged":[]}
["VIQ_ref_no","Risk Value of observation","ID"]
["1.1","Low",8243]
["1.10","Low",8252]
["1.11","Low",8253]
["1.12","Low",8254]
["1.13","Low",8255]
["1.14","Low",8256]
["1.15","Low",8257]
["1.16","Low",8259]
["1.17","Low",8260]
["1.18","Low",8261]
["1.19","Low",8262]
["1.2","Low",8244]
["1.20","Low",8263]
["1.21","Low",8265]
["1.22","Low",8266]
["1.23","Low",8267]
["1.24","Low",8268]
["1.25","Low",8269]
["1.26","Low",8270]
["1.3","Low",8245]
["1.4","Low",8246]
["1.5","Low",8247]
["1.6","Low",8248]
["1.7","Low",8249]
["1.8","Low",8250]
["1.9","Low",8251]
["1.99","High",11258]
["10.1","Medium",8461]
["10.10","High",8470]
["10.11","Medium",8471]
["10.12","Very High",8472]
["10.13","Very High",8473]
["10.14","Medium",8474]
["10.15","Low",8475]
["10.16","Very High",8476]
["10.17","Very High",8477]
["10.18","High",8478]
["10.19","Very High",8479]
["10.2","Low",8462]
["10.20","High",8480]
["10.21","Medium",8481]
["10.22","Low",8482]
["10.23","Medium",8483]
["10.24","Low",8484]
["10.25","Very High",8485]
["10.26","High",8486]
["10.27","Medium",8487]
["10.28","Low",8488]
["10.29","Medium",8489]
["10.3","Medium",8463]
["10.30","High",8490]
["10.31","Very High",8491]
["10.32","Very High",8492]
["10.33","High",8493]
["10.34","High",8494]
["10.35","Very High",8495]
["10.36","Very High",8496]
["10.37","Medium",8497]
["10.38","Medium",8498]
["10.39","High",8499]
["10.4","High",8464]
["10.40","Medium",8500]
["10.41","Medium",8501]
["10.42","Medium",8502]
["10.43","Medium",8503]
["10.44","Medium",8504]
["10.45","Very High",8505]
["10.46","High",8506]
["10.47","Medium",8507]
["10.48","High",8508]
["10.49","Medium",8509]
["10.5","Low",8465]
["10.50","High",8510]
["10.51","Low",8511]
["10.52","Medium",8512]
["10.53","Medium",8513]
["10.54","High",8514]
["10.55","Low",8515]
["10.6","Very High",8466]
["10.7","Medium",8467]
["10.8","Medium",8468]
["10.9","Medium",8469]
["10.99","High",8516]
["11.1","High",8420]
["11.10","Medium",8429]
["11.11","Very High",8430]
["11.12","Low",8431]
["11.13","Low",8432]
["11.14","Medium",8433]
["11.15","Low",8434]
["11.16","Low",8435]
["11.17","Low",8436]
["11.2","Medium",8421]
["11.3","Medium",8422]
["11.4","Very High",8423]
["11.5","Medium",8424]
["11.6","Medium",8425]
["11.7","High",8426]
["11.8","Low",8427]
["11.9","Low",8428]
["11.99","High",8437]
["12.1","High",8438]
["12.10","High",8448]
["12.11","High",8449]
["12.12","High",8450]
["12.13","High",8451]
["12.14","High",8452]
["12.15","High",8453]
["12.16","High",8454]
["12.17","High",8455]
["12.18","High",8456]
["12.19","High",8457]
["12.2","High",8439]
["12.20","High",8458]
["12.21","High",8459]
["12.3","High",8441]
["12.4","High",8442]
["12.5","High",8443]
["12.6","High",8444]
["12.7","High",8445]
["12.8","High",8446]
["12.9","High",8447]
["12.99","High",8460]
["2.1","Very High",8296]
["2.1.9","Very High",11259]
["2.10","Medium",8304]
["2.11","Medium",8305]
["2.12","Low",8306]
["2.13","Low",8307]
["2.14","Low",8308]
["2.15","Low",8309]
["2.16","Medium",8310]
["2.2","Medium",8297]
["2.3","High",8295]
["2.4","Medium",8298]
["2.5","Medium",8299]
["2.6","Low",8300]
["2.7","High",8301]
["2.8","High",8302]
["2.9","Medium",8303]
["2.99","High",8311]
["3.1","High",8312]
["3.2","Very High",8313]
["3.3","High",8314]
["3.4","Low",8294]
["3.5","Medium",8315]
["3.6","High",8316]
["3.7","Very High",8317]
["3.8","Very High",8318]
["3.99","High",8319]
["4.1","High",8320]
["4.10","High",8329]
["4.11","Medium",8330]
["4.12","Very High",8331]
["4.13","Very High",8332]
["4.14","Very High",8333]
["4.15","Very High",8334]
["4.16","Very High",8335]
["4.17","Very High",8336]
["4.18","Very High",8337]
["4.19","Low",8338]
["4.2","Medium",8321]
["4.20","Very High",8339]
["4.21","High",8340]
["4.22","Low",8341]
["4.23","High",8342]
["4.24","High",8343]
["4.25","Low",8344]
["4.26","Low",8345]
["4.27","High",8346]
["4.3","Medium",8322]
["4.4","High",8323]
["4.5","Very High",8324]
["4.6","Medium",8325]
["4.7","High",8326]
["4.8","Medium",8327]
["4.9","Medium",8328]
["4.99","High",8347]
["5.1","Very High",8517]
["5.10","High",8526]
["5.11","Low",8527]
["5.12","Medium",8528]
["5.13","High",8529]
["5.14","Very High",8530]
["5.15","Medium",8531]
["5.16","Very High",8532]
["5.17","Very High",8533]
["5.18","High",8534]
["5.19","Medium",8535]
["5.2","Very High",8518]
["5.20","Medium",8536]
["5.21","Medium",8537]
["5.22","High",8539]
["5.23","Very High",8540]
["5.24","Very High",8541]
["5.25","Medium",8542]
["5.26","Medium",8543]
["5.27","Medium",8544]
["5.28","Very High",8545]
["5.29","High",8546]
["5.3","Low",8519]
["5.30","High",8547]
["5.31","High",8548]
["5.32","High",8549]
["5.33","High",8550]
["5.34","Low",8551]
["5.35","Medium",8552]
["5.36","Low",8553]
["5.37","Low",8554]
["5.38","High",8555]
["5.39","Very High",8556]
["5.4","High",8520]
["5.40","Very High",8557]
["5.41","Very High",8558]
["5.42","Medium",8559]
["5.43","High",8560]
["5.44","High",8561]
["5.45","Medium",8564]
["5.46","Medium",8565]
["5.47","Medium",8566]
["5.48","Medium",8567]
["5.5","Low",8521]
["5.6","Low",8522]
["5.7","Medium",8523]
["5.8","Medium",8524]
["5.9","Very High",8525]
["5.99","High",8568]
["6.1","Medium",8348]
["6.10","Low",8357]
["6.11","High",8358]
["6.12","Medium",8359]
["6.13","Low",8360]
["6.14","High",8361]
["6.15","High",8362]
["6.16","Very High",8363]
["6.17","Very High",8364]
["6.18","Medium",8365]
["6.19","Low",8366]
["6.2","High",8349]
["6.20","Medium",8367]
["6.21","High",8368]
["6.22","Medium",8369]
["6.3","Low",8350]
["6.4","High",8351]
["6.5","Medium",8352]
["6.6","Medium",8353]
["6.7","High",8354]
["6.8","High",8355]
["6.9","Low",8356]
["6.99","High",8370]
["7.1","High",8371]
["7.10","High",8380]
["7.11","High",8381]
["7.12","High",8382]
["7.13","Medium",8383]
["7.14","Medium",8384]
["7.15","High",8385]
["7.16","High",8386]
["7.17","High",8387]
["7.2","High",8372]
["7.3","Low",8373]
["7.4","Low",8374]
["7.5","Low",8375]
["7.6","Medium",8376]
["7.7","Low",8377]
["7.8","High",8378]
["7.9","High",8379]
["7.99","High",8388]
["8.1","Very High",8569]
["8.10","Very High",8578]
["8.100","Low",11227]
["8.101","Medium",11228]
["8.102","Low",11229]
["8.103","Low",11230]
["8.104","Low",11231]
["8.105","Medium",11232]
["8.106","Medium",11233]
["8.107","Low",11234]
["8.108","High",11235]
["8.109","Very High",11236]
["8.11","Medium",8579]
["8.110","High",11237]
["8.111","Medium",11238]
["8.112","High",11239]
["8.113","Medium",11240]
["8.114","Low",11241]
["8.115","High",11242]
["8.116","Medium",11243]
["8.117","Medium",11244]
["8.118","Medium",11245]
["8.119","High",11246]
["8.12","Medium",8580]
["8.120","High",11247]
["8.121","Medium",11248]
["8.122","High",11249]
["8.123","High",11250]
["8.124","Low",11251]
["8.125","High",11252]
["8.126","Medium",11253]
["8.127","Medium",11254]
["8.13","Medium",8581]
["8.14","Very High",8582]
["8.15","High",8583]
["8.16","Very High",8584]
["8.17","Low",8585]
["8.18","High",8586]
["8.19","High",8587]
["8.199","High",11255]
["8.2","Medium",8570]
["8.20","Medium",8588]
["8.21","High",8589]
["8.22","Very High",8590]
["8.23","Medium",8591]
["8.24","Medium",8592]
["8.25","Very High",8593]
["8.26","High",8594]
["8.27","Medium",8595]
["8.28","Medium",8596]
["8.29","High",8598]
["8.3","Very High",8571]
["8.30","High",8599]
["8.31","High",8600]
["8.32","Low",8601]
["8.33","Medium",8602]
["8.34","High",8603]
["8.35","Medium",8604]
["8.36","Medium",8605]
["8.37","High",8607]
["8.38","Medium",8608]
["8.39","Medium",8609]
["8.4","Medium",8572]
["8.40","High",8610]
["8.41","Medium",8611]
["8.42","Medium",8612]
["8.43","Very High",8613]
["8.44","High",8615]
["8.45","High",8616]
["8.46","Very High",8617]
["8.47","Very High",8618]
["8.48","Medium",8619]
["8.49","High",8620]
["8.5","Very High",8573]
["8.50","Medium",8621]
["8.51","Low",8622]
["8.52","Low",8623]
["8.53","Low",8624]
["8.54","High",8625]
["8.55","Low",11182]
["8.56","Medium",11183]
["8.57","Medium",11184]
["8.58","High",11185]
["8.59","High",11186]
["8.6","Medium",8574]
["8.60","High",11187]
["8.61","Medium",11188]
["8.62","Very High",11189]
["8.63","High",11190]
["8.64","Medium",11191]
["8.65","Low",11192]
["8.66","High",11193]
["8.67","High",11194]
["8.68","High",11195]
["8.69","Medium",11196]
["8.7","High",8575]
["8.70","Medium",11197]
["8.71","Very High",11198]
["8.72","Medium",11199]
["8.73","Medium",11200]
["8.74","High",11201]
["8.75","Medium",11202]
["8.76","Medium",11203]
["8.77","Medium",11204]
["8.78","Medium",11205]
["8.79","Medium",11206]
["8.8","Medium",8576]
["8.80","Medium",11207]
["8.81","Low",11208]
["8.82","Medium",11209]
["8.83","Low",11210]
["8.84","Low",11211]
["8.85","Medium",11212]
["8.86","Medium",11213]
["8.87","Medium",11214]
["8.88","Low",11215]
["8.89","High",11216]
["8.9","High",8577]
["8.90","High",11217]
["8.91","High",11218]
["8.92","Medium",11219]
["8.93","Low",11220]
["8.94","Low",11221]
["8.95","Medium",11222]
["8.96","Medium",11223]
["8.97","Low",11224]
["8.98","High",11225]
["8.99","Medium",11226]
["9.1","Low",8390]
["9.10","Medium",8399]
["9.11","Medium",8400]
["9.12","Medium",8401]
["9.13","Low",8402]
["9.14","Medium",8403]
["9.15","Medium",8404]
["9.16","High",8405]
["9.17","High",8406]
["9.18","Low",8407]
["9.19","Low",8408]
["9.2","Very High",8391]
["9.20","Medium",8409]
["9.21","Medium",8410]
["9.22","Low",8411]
["9.23","Low",8412]
["9.24","Medium",8413]
["9.25","Low",8414]
["9.26","Low",8415]
["9.27","Low",8416]
["9.28","Medium",8417]
["9.29","Low",8418]
["9.3","Very High",8392]
["9.4","High",8393]
["9.5","High",8394]
["9.6","Low",8395]
["9.7","Medium",8396]
["9.8","Medium",8397]
["9.9","Medium",8398]
["9.99","High",8419]

{"sheet":"Equipment_list","index":7,"n_rows":28,"n_cols":3,"rows_kept":28,"cut":false,"hidden":true,"merged":[]}
["TITLE","Equipment_list_description","ID"]
["Accommodation",null,12]
["Cargo Mach.",null,13]
["Critical Equip.",null,16]
["Deck - Machinery",null,18]
["Deck - Mooring Machinery",null,15]
["Deck - Pipe / Fittings",null,20]
["Documentation",null,21]
["E/R - Air Comp.",null,8]
["E/R - Aux. Engine",null,4]
["E/R - Aux. Mach.",null,7]
["E/R - Boiler",null,5]
["E/R - Main Engine",null,3]
["E/R - Pipes/ valves & fittings",null,9]
["E/R - Pumps",null,32]
["E/R - Purifier",null,6]
["Elect. Mach. & Equip.",null,10]
["Hull & Tanks",null,19]
["Inert Gas",null,14]
["LSA / FFA",null,17]
["Miscellaneous",null,22]
["Navigation - DGPS / EPFS / AIS",null,28]
["Navigation - ECDIS",null,25]
["Navigation - Echo Sounder / Speed Log",null,26]
["Navigation - GMDSS & Communication",null,23]
["Navigation - Others",null,11]
["Navigation - RADAR",null,24]
["Navigation - VDR / BNWAS",null,30]

{"sheet":"PSC_MOU","index":8,"n_rows":11,"n_cols":3,"rows_kept":11,"cut":false,"hidden":true,"merged":[]}
["TITLE","PSC_MOU_description","ID"]
["Asia and the Pacific",null,2]
["Caribbean",null,4]
["Europe and the North Atlantic",null,1]
["Latin America",null,3]
["The Black Sea region",null,6]
["The Indian Ocean",null,8]
["The Mediterranean",null,7]
["The Riyadh MoU",null,9]
["USCG",null,10]
["West and Central Africa",null,5]

{"sheet":"Inspection_type","index":9,"n_rows":13,"n_cols":2,"rows_kept":13,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Bunkering Audit",14]
["Cargo Audit",17]
["Engineering Audit",16]
["ISM Audit",2]
["ISPS Audit",3]
["IT Audit",10]
["MLC Audit",1]
["Mooring Audit",9]
["Nav Audit / Verification",8]
["Onboard Training",18]
["Ship Staff Insp.",15]
["Suptd. Insp.",13]

{"sheet":"Deficiency_Cause","index":10,"n_rows":8,"n_cols":3,"rows_kept":8,"cut":false,"hidden":true,"merged":[]}
["TITLE","Deficiency_Cause_description","ID"]
["Behaviour Based",null,1]
["Equipment Related",null,4]
["External Factors",null,5]
["Human Error",null,7]
["Inappropriate Procedure",null,8]
["Industry Issue",null,6]
["Knowledge Based",null,3]

{"sheet":"Observer_code","index":11,"n_rows":3,"n_cols":3,"rows_kept":3,"cut":false,"hidden":true,"merged":[]}
["TITLE","Observer_code_description","ID"]
["Owner / Marine / Tech. Suptd.",null,3]
["Ship Staff",null,2]

{"sheet":"Status_code","index":12,"n_rows":6,"n_cols":3,"rows_kept":6,"cut":false,"hidden":true,"merged":[]}
["TITLE","Status_code_description","ID"]
["Completed",null,6]
["Deferred to D D",null,5]
["In progress",null,3]
["Not Started",null,2]
["Waiting spare",null,4]

{"sheet":"PSC_ref_no","index":13,"n_rows":19,"n_cols":2,"rows_kept":19,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Alarms",9]
["Cargo operations including equipment",7]
["Certificates & Documentation",2]
["Dangerous Goods",13]
["Emergency Systems",5]
["Fire safety",8]
["ISM",16]
["ISPS",17]
["Life saving appliances",12]
["MLC, 2006",18]
["Other",19]
["Pollution Prevention",15]
["Propulsion and auxiliary machinery",14]
["Radio communication",6]
["Safety of Navigation",11]
["Structural condition",3]
["Water/Weathertight condition",4]
["Working and Living Conditions",10]

{"sheet":"Risk_value_of_obs","index":14,"n_rows":1,"n_cols":2,"rows_kept":1,"cut":false,"hidden":true,"merged":[]}
["Risk Value of observation","ID"]

{"sheet":"Year","index":15,"n_rows":18,"n_cols":1,"rows_kept":18,"cut":false,"hidden":true,"merged":[]}
["Year"]
[2014]
[2015]
[2016]
[2017]
[2018]
[2019]
[2020]
[2021]
[2022]
[2023]
[2024]
[2025]
[2026]
[2027]
[2028]
[2029]
[2030]

{"sheet":"Month","index":16,"n_rows":13,"n_cols":1,"rows_kept":13,"cut":false,"hidden":true,"merged":[]}
["Month"]
["Jan"]
["Feb"]
["Mar"]
["Apr"]
["May"]
["Jun"]
["Jul"]
["Aug"]
["Sep"]
["Oct"]
["Nov"]
["Dec"]

{"sheet":"Date_","index":17,"n_rows":32,"n_cols":1,"rows_kept":32,"cut":false,"hidden":true,"merged":[]}
["Date"]
["01"]
["02"]
["03"]
["04"]
["05"]
["06"]
["07"]
["08"]
["09"]
[10]
[11]
[12]
[13]
[14]
[15]
[16]
[17]
[18]
[19]
[20]
[21]
[22]
[23]
[24]
[25]
[26]
[27]
[28]
[29]
[30]
[31]

{"sheet":"Sheet1","index":18,"n_rows":24,"n_cols":6,"rows_kept":24,"cut":false,"hidden":true,"merged":[]}
[]
[null,"ID","E",null,"Date Recorded",1]
[null,"UNIQUE ID","F",null,"Type of Deficiency",2]
[1,"Date Recorded","G",null,"Observer code",3]
["ignore","Vessel Type","H",null,"Type of Inspection",4]
[null,"Internal / External","I",null,"Description of Deficiency",5]
[null,"Drydock","J",null,"Equipment Categories",6]
[null,"Information Sharing","K",null,"Area of Observation",7]
[null,"Critical_item","L",null,"Deficiency Cause",8]
[null,"Deficiency Type","M",null,"VIQ Ref Number",9]
[null,"Deficiency Cause","N",null,"Risk Value of Obs",10]
[null,"Inspection Type","O",null,"PSC Ref Number",11]
[null,"Equipments","P",null,"PSC MOU ID",12]
[null,"VIQ Reference Number","Q",null,"Action Taken or Required",13]
[null,"Risk Value of the observation","R",null,"Target Date",14]
[null,"PSC Reference Number","S",null,"PO Ref No.",15]
[null,"PSC MOU","T",null,"Status Code",16]
[null,"Observer Code","U",null,"Date Completed",17]
[null,"Target Date","V",null,"Drydock",18]
[null,"Status Code","W",null,"Info Sharing",19]
[null,"Description of Deficiency","X",null,"Critical Item Flag",20]
[null,"Action taken / required","Y",null,"Audit Type",21]
[null,"PO ref no","Z"]
[null,"Date completed","AA"]

{"sheet":"Ship_information","index":19,"n_rows":2,"n_cols":4,"rows_kept":2,"cut":false,"hidden":true,"merged":[]}
["Ship_ID","Ship_Name","FILE_NAME","Export_Date"]
["55","DHT SUNDARBANS (05-12-2023)","55_1704692174940.xlsm","2024-03-16 00:03:38"]

{"sheet":"External_Deficiency_type","index":20,"n_rows":5,"n_cols":3,"rows_kept":5,"cut":false,"hidden":true,"merged":[]}
["TITLE","Type of deficiency_description","ID"]
["Condn of Class / Memo",null,5]
["Defect",null,1]
["Non Conformity",null,2]
["Observation",null,3]

{"sheet":"External_Inspection_type","index":21,"n_rows":11,"n_cols":2,"rows_kept":11,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Cargo Audit",17]
["Flag State Insp.",5]
["ISM Audit",2]
["ISPS Audit",3]
["MLC Audit",1]
["Nav Audit / Verification",8]
["OM Insp. (Eg. SIRE / CDI etc.)",6]
["Others (Eg. Insurance etc.)",12]
["PSC Inspection",4]
["Terminal Insp.",11]

{"sheet":"External_Observer_code","index":22,"n_rows":7,"n_cols":3,"rows_kept":7,"cut":false,"hidden":true,"merged":[]}
["TITLE","Observer_code_description","ID"]
["Class Surveyor",null,4]
["FSC Inspector",null,5]
["Others (Eg. Insurance etc.)",null,9]
["PSC Insp.",null,6]
["SIRE / CDI Insp.",null,8]
["Terminal Insp.",null,7]

{"sheet":"Sheet Version","index":23,"n_rows":2,"n_cols":2,"rows_kept":2,"cut":false,"hidden":true,"merged":[]}
["Version","Title"]
["2.0","Version 2.0"]