{"text_format":"1","workbook":"xlsx","n_sheets":24,"sheets":["Mainsheet","Completed","Calc","Areaofobs","Vessel_type","Deficiency_type","VIQrefno","Equipment_list","PSC_MOU","Inspection_type","Deficiency_Cause","Observer_code","Status_code","PSC_ref_no","Risk_value_of_obs","Year","Month","Date_","Sheet1","Ship_information","External_Deficiency_type","External_Inspection_type","External_Observer_code","Sheet Version"],"not_rendered":{"charts":0,"images":1,"macros":1,"external_links":0,"defined_names":12,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Mainsheet","index":0,"n_rows":18,"n_cols":28,"rows_kept":18,"cut":false,"hidden":false,"merged":[[10,8,10,9],[10,12,10,13],[12,6,12,27],[8,6,8,27]]}
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,"Defect - Damage Monitoring Sheet"]
[]
[null,null,null,null,null,null,null,"Date of Report","01-May-2024",null,null,"Ship Name","PELAGOS (03-04-2024)"]
[]
[null,null,null,null,null,null,"VERSION : 2.0"]
[]
[]
[]
[null,null,null,"ID","SHIPSIDE UNIQUEID","UNIQUE ID","Date Recorded","Type of Deficiency","Observer code","Type of Inspection","Description of Deficiency","Equipment Categories","Area of Observation","Deficiency Cause","VIQ Ref Number","Risk Value of Obs","PSC Ref Number","PSC MOU ID","Action Taken or Required","Target Date","PO Ref No.","Status Code","Date Completed","Drydock","Info Sharing","Critical Item","Audit Type","Superintendent Remarks"]
[null,null,null,null,19806,"123_Wed Nov 15 2023 19:27:36 GMT+0800","2024-01-02T08:00:00","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Rubber pads/cushion on all cover hatch cover stopper plate, 60 in number to be replaced with new once received","Cargo Mach.","Cargo / Ballast Systems","External Factors","","","","","Replace new rubber cushion of all hatch cover stopper plate.","2024-05-15T08:00:00","","Not Started",null,"No","No","No","Internal","Replace with new rubber cushion during ballast passage."]

{"sheet":"Completed","index":1,"n_rows":354,"n_cols":28,"rows_kept":354,"cut":false,"hidden":false,"merged":[[10,8,10,9],[10,12,10,13],[12,6,12,27],[8,6,8,27]]}
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,"Defect - Damage Monitoring Sheet"]
[]
[null,null,null,null,null,null,null,"Date of Report","01-May-2024",null,null,"Ship Name","PELAGOS (03-04-2024)"]
[]
[null,null,null,null,null,null,"VERSION : 2.0"]
[]
[]
[]
[null,null,null,"ID","SHIPSIDE UNIQUEID","UNIQUE ID","Date Recorded","Type of Deficiency","Observer code","Type of Inspection","Description of Deficiency","Equipment Categories","Area of Observation","Deficiency Cause","VIQ Ref Number","Risk Value of Obs","PSC Ref Number","PSC MOU ID","Action Taken or Required","Target Date","PO Ref No.","Status Code","Date Completed","Drydock","Info Sharing","Critical Item","Audit Type","Superintendent Remarks"]
[null,null,null,21116,null,"123_16/9/2021 9:35:02 pm","2021-08-17T23:59:35","Defect","Ship Staff","Ship Staff Insp.","PORT USE PUMP UN ABLE TO GIIVE SUCTION AND DICHARGE PRESSURE ","E/R - Pumps","ISM Related","Equipment Related","","","","","OVERHAULED PUMP REPLACE DEFECTIVE IMPELLER, WEAR RING , SUBMERGE BUSH BEARING.","2021-09-14T23:59:35","","Completed","2021-09-14T23:59:35","No","No","No","Internal"]
[null,null,null,22870,null,"123_31/10/2021 8:56:30 pm","2021-08-19T23:59:35","Non Conformity","Ship Staff","Ship Staff Insp.","Departing Manilawith in complete ENC permit of the intended passage/voyage","Navigation - ECDIS","Navigation","Knowledge Based","","","","","Inquire assistance to Navtor & Office. Training to responsible officer","2021-08-26T23:59:35","","Completed","2021-08-22T23:59:35","No","No","No","Internal"]
[null,null,null,21117,null,"123_16/9/2021 2:01:49 am","2021-08-19T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Departing Manila with incomplete ENC Permit of the intended passage/voyage.","Navigation - ECDIS","Navigation","Knowledge Based","","","","","Inquire assistance to IT and Navtor Provider to provide missing ENC permit. Training and familiarization carried out to all officers. Advised to Nav. Officer to make an advance inquiry of ENC permit for the next intended voyage as the external internet communication (Data Connection) very slow.","2021-08-24T23:59:35","","Completed","2021-08-22T23:59:35","No","No","No","Internal"]
[null,null,null,21118,null,"123_7/9/2021 12:32:03 pm","2021-08-26T23:59:35","Defect","Ship Staff","Ship Staff Insp.","No. 2 Marine Radar ARPA (X-Band) was 4 Times replace the fuse but same before Fuse Element was busted. We suspected the PCB Electronics Parts of CPU, TB Board, Control Unit, Power Supply Unit & other Electronics Parts was Damage & Broken.","Navigation - RADAR","Navigation","Equipment Related","","","","","Informed Office and Shore's Assistance","2021-09-26T23:59:35","","Completed","2021-09-10T23:59:35","No","No","No","Internal"]
[null,null,null,21115,null,"123_15/9/2021 9:18:22 pm","2021-08-27T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Holed pipe of ME FW cooler seawater outlet sarificial pipe.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Replaced with new pipe and flange.","2021-09-06T23:59:35","","Completed","2021-09-06T23:59:35","No","No","No","Internal"]
[null,null,null,21119,null,"123_15/9/2021 9:31:53 pm","2021-08-27T23:59:35","Defect","Ship Staff","Ship Staff Insp.","ME FW cooler seawater sacrificial inlet pipe leak on seam side.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Repair by welding seam portion of the pipe, since the pipe is still in good condition and its thickness.","2021-09-06T23:59:35","","Completed","2021-09-06T23:59:35","No","No","No","Internal"]
[null,null,null,21121,null,"123_15/9/2021 9:48:29 pm","2021-08-27T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Main Cooling SW pump no.2 Sacrificial pipe at suction side leak.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Replaced with new pipe and flange.","2021-09-06T23:59:35","","Completed","2021-09-06T23:59:35","No","No","No","Internal"]
[null,null,null,21120,null,"123_7/9/2021 12:08:59 pm","2021-09-05T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Radar S-Band Observed Poor sensitivity & Echo","Navigation - RADAR","Navigation","Equipment Related","","","","","Inquire Office and Maker Assistance or Shore's Service Technician at Next Port","2021-10-05T23:59:35","","Completed","2021-09-10T23:59:35","No","No","No","Internal"]
[null,null,null,21112,null,"123_16/9/2021 2:14:52 am","2021-09-07T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Both ECDIS unable to save route plan and load new route plan in ECDIS monitor ","Navigation - ECDIS","Navigation","Equipment Related","","","","","Inquires assistance to office and Maker","2021-10-07T23:59:35","","Completed","2021-09-09T23:59:35","No","No","No","Internal"]
[null,null,null,22879,null,"123_31/10/2021 9:00:35 pm","2021-09-21T23:59:35","Non Conformity","Ship Staff","Ship Staff Insp.","Some missing entry in Deck Log Book","Documentation","Cert. & Docu.","Knowledge Based","","","","","Briefing/Training carried out to all OOW.","2021-10-29T23:59:35","","Completed","2021-09-29T23:59:35","No","No","No","Internal"]
[null,null,null,22863,null,"123_20/9/2021 2:38:06 pm","2021-09-27T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Wear down of impeller and leakage on pump body due to mechanical seal damage.","E/R - Boiler,E/R - Pumps","ISM Related","Equipment Related","","","","","Overhauled and checked.Need to replace the damage mechanical seal and impeller as a set. We request  spare  for replacement.","2021-10-30T23:59:35","PELA210059 BOILER FEED PUMP","Completed","2021-12-09T23:59:35","No","No","No","Internal"]
[null,null,null,22880,null,"123_30/9/2021 9:54:24 pm","2021-09-29T23:59:35","Defect","Ship Staff","Ship Staff Insp.","DE-SYNCHRONIZATION OF DG NO.1 WAS NOT ABLE AND WE FOUND OUT THAT THE WOODWARD APM MOTOR CONTROL WAS BURNT LOCATED AT DG NO 1 MAIN CONTROL PANEL AT ER CONTROL ROOM.","E/R - Aux. Engine","ISM Related","Equipment Related","","","","","CARRIED OUT MANUALLY DE-SYNCHRONIZATION AND CHECKED THE APM MOTOR / FOUND BURNT. SECURE DG NO.1 / NEEDED TOTAL REPLACEMENT OF APM MOTOR CONTROL.","2021-12-29T23:59:35","PO Ref No. PELA210063","Completed","2021-10-28T23:59:35","No","No","No","Internal"]
[null,null,null,22865,null,"123_31/10/2021 9:17:53 pm","2021-10-24T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","FPT Water Ingress Alarm Sensor Defective","Miscellaneous","Structural Condn. / WT integrity ","Equipment Related","","","","","replaced with new spare PCB / now in good working condition.","2022-01-24T23:59:35","PELA210085","Completed","2021-12-08T23:59:35","No","No","No","Internal"]
[null,null,null,22866,null,"123_31/10/2021 9:37:01 pm","2021-10-24T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Low insulation found in 440V & 220V on MSB","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","Informed Office and Identify Caused and rectify","2021-12-24T23:59:35","","Completed","2021-10-26T23:59:35","No","No","No","Internal"]
[null,null,null,22871,null,"123_31/10/2021 9:55:24 pm","2021-10-24T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Rust & Difficult to open the steering mushroom vent head in poop deck","Deck - Pipe / Fittings","General Appearance","Equipment Related","","","","","Derusted, freed and painted","2022-01-24T23:59:35","","Completed","2021-10-25T23:59:35","No","No","No","Internal"]
[null,null,null,22872,null,"123_31/10/2021 9:47:54 pm","2021-10-24T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Heavy rust found in watertight door edges where the gasket in place in steering, CO2 Room and emergency exit watertight door","Miscellaneous","Structural Condn. / WT integrity ","Equipment Related","","","","","Derusted and painted","2022-01-24T23:59:35","","Completed","2021-10-25T23:59:35","No","No","No","Internal"]
[null,null,null,22896,null,"123_2/12/2021 9:04:14 pm","2021-10-24T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ER Bilge/OWS pipelines not sealed as per Company Policy, same to be carried out & form filled","E/R - Pipes/ valves & fittings","MARPOL Related","Knowledge Based","","","","","ER Bilge/OWS Pipelines Flanges sealed as per Compancy Policy and form filled","2021-10-29T23:59:35","","Completed","2021-10-26T23:59:35","No","No","No","Internal"]
[null,null,null,22897,null,"123_2/12/2021 9:22:48 pm","2021-10-24T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ER ORB not countersigned by officer incharge","E/R - Pipes/ valves & fittings","MARPOL Related","Knowledge Based","","","","","Briefed and advised to officer incharge to countersigned ER ORB entry not only C/E for strict compliance.","2021-10-27T23:59:35","","Completed","2021-10-24T23:59:35","No","No","No","Internal"]
[null,null,null,22898,null,"123_2/12/2021 9:27:02 pm","2021-10-24T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","One of the ER DB Tank Sounding CAP missing, same to be always fixed","E/R - Pipes/ valves & fittings","MARPOL Related","Knowledge Based","","","","","Put back sounding cap and fixed. Briefed all rating and Eng'r to make sure all sounding CAP to be put back and fixed after used accordingly.","2021-10-25T23:59:35","","Completed","2021-10-24T23:59:35","No","No","No","Internal"]
[null,null,null,22899,null,"123_2/12/2021 9:39:15 pm","2021-10-24T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Fingersavers & impact gloves not placed in ER workshop for quick availability","LSA / FFA","Safety / LSA / FFA","Knowledge Based","","","","","Fingersavers & impact gloves handed over to 2E to place in ER workshop","2021-10-29T23:59:35","","Completed","2021-10-26T23:59:35","No","No","No","Internal"]
[null,null,null,22900,null,"123_2/12/2021 9:51:51 pm","2021-10-24T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Incinerator electrical panel found dirty, same to be soap washed","Elect. Mach. & Equip.","General Appearance","Knowledge Based","","","","","Instructed Engine rating to clean and soap washed Incinerator electrical panel","2021-10-29T23:59:35","","Completed","2021-10-25T23:59:35","No","No","No","Internal"]
[null,null,null,22901,null,"123_2/12/2021 9:56:49 pm","2021-10-24T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Deck walkway and snap back zone yellow mark faded and peel off. need to repaint","Miscellaneous","General Appearance","External Factors","","","","","Repainted faded and peel off yellow mark in Deck walkway and snap back zone ","2021-11-24T23:59:35","","Completed","2021-11-08T23:59:35","No","No","No","Internal"]
[null,null,null,22902,null,"123_2/12/2021 10:03:51 pm","2021-10-24T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Isolated Heavy rust found underneath of deck fire line. Need to derust and paint ore replace new pipe if needed","Deck - Pipe / Fittings","General Appearance","External Factors","","","","","Derusted and painted.","2022-01-24T23:59:35","","Completed","2021-11-30T23:59:35","No","No","No","Internal"]
[null,null,null,22903,null,"123_2/12/2021 10:25:08 pm","2021-10-24T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Some Markings on deck faded, need to redo the stenciling","Miscellaneous","General Appearance","External Factors","","","","","Restenciling deck faded marking","2021-11-03T23:59:35","","Completed","2021-11-02T23:59:35","No","No","No","Internal"]
[null,null,null,22904,null,"123_2/12/2021 10:30:12 pm","2021-10-24T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Steering gear chemical locker to square up and arrange not to mix or close the alkaline and acid","Miscellaneous","Safety / LSA / FFA","Knowledge Based","","","","","Square up neatly and separate alkaline and acid.","2021-10-29T23:59:35","","Completed","2021-10-25T23:59:35","No","No","No","Internal"]
[null,null,null,22905,null,"123_2/12/2021 10:37:42 pm","2021-10-24T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Hook latche defective of general use handling crane, provision crane and hose handling crane. To repair/fabricate hook latche spring","Deck - Machinery","Safety / LSA / FFA","Equipment Related","","","","","Hook lacthe spring fabricated","2021-11-03T23:59:35","","Completed","2021-10-25T23:59:35","No","No","No","Internal"]
[null,null,null,21114,null,"123_15/9/2021 8:15:37 pm","2021-10-24T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Marine Type Packaged Air Conditioner for Galley observed no output air cooling in the Galley even though the Thermostat Knob Controller was in the Maximum Cold Point.","Accommodation","MLC Related","Equipment Related","","","","","We Pump down the system & no collected Refrigerant Gas Freon was seen. We performed leak test by liquid soap mixed with water, Ref. Gas Leak Detector, Vacuum Pump & we found out multiple leakage in the Evaporator Unit. In the Evaporator the Air Suction Grilled was rusted, corroded & eliminated. Create RO for the whole 1 set of Evaporator. Received spare and installed","2021-12-09T23:59:35","","Completed","2021-11-30T23:59:35","No","No","No","Internal"]
[null,null,null,22873,null,"123_31/10/2021 10:50:32 pm","2021-10-27T23:59:35","Non Conformity","FSC Inspector","Flag State Insp.","Cew Rat#17 Mr Porras - STCW VI/2.1 Expired 04 Sep 2021","Documentation","Cert. & Docu.","Knowledge Based","","","","","Inquired confirmation to Manning Office if it is mandatory to renew/have the said National Certificate or not as per STCW and Liberian Flag State requirements. They confirmed is not mandatory of his rank.","2021-11-27T23:59:35","","Completed","2021-10-29T23:59:35","No","No","No","External"]
[null,null,null,22874,null,"123_31/10/2021 10:55:07 pm","2021-10-27T23:59:35","Non Conformity","FSC Inspector","Flag State Insp.","Recovery of Person from water manual section 10 - not filled with ships specific information required by company","Documentation","ISM Related","Knowledge Based","","","","","Immediately inserted the required list of ship specific information in the manual.","2021-11-27T23:59:35","","Completed","2021-10-27T23:59:35","No","No","No","External"]
[null,null,null,22875,null,"123_31/10/2021 10:58:57 pm","2021-10-27T23:59:35","Non Conformity","FSC Inspector","Flag State Insp.","Following Pubs outdated w/no access to electronic: IMDG Code, SOLAS, IMSBC","Documentation","ISM Related","Knowledge Based","","","","","Immediate raised requisition for the new edition ","2021-11-09T23:59:35","PELA215045","Completed","2021-11-02T23:59:35","No","No","No","External"]
[null,null,null,22876,null,"123_31/10/2021 11:03:11 pm","2021-10-27T23:59:35","Observation","FSC Inspector","Flag State Insp.","Poop Dk-S/S; Mooring Winch (Outb)-Brake Lining very poor condition","Deck - Mooring Machinery","Mooring","Equipment Related","","","","","Replace new brake lining","2021-11-07T23:59:35","","Completed","2021-11-05T23:59:35","No","No","No","External"]
[null,null,null,22877,null,"123_31/10/2021 11:07:52 pm","2021-10-28T23:59:35","Non Conformity","Others (Eg. Insurance etc.)","Others (Eg. Insurance etc.)","Vessel's security checkpoint unmanned at time surveyor boarded.","Miscellaneous","ISPS Related","Knowledge Based","","","","","Immediate training/briefing to all officers and deck crew for strict compliance of ISPS requirements. Don't ever left vessel security checkpoint at all times.","2021-10-28T23:59:35","","Completed","2021-10-28T23:59:35","No","No","No","External"]
[null,null,null,22878,null,"123_13/11/2021 11:12:55 pm","2021-11-10T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Freefall lifeboat rudder slight dented","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","Remove and straighten the rudder ","2021-11-29T23:59:35","","Completed","2021-11-12T23:59:35","No","No","No","Internal"]
[null,null,null,22881,null,"123_1/12/2021 11:22:03 pm","2021-11-12T23:59:35","Non Conformity","Ship Staff","Ship Staff Insp.","Fire hose that was used during the fire drill found not secure after drill, was observed on the next day when safety rounds/check conducted.","LSA / FFA","Safety / LSA / FFA","Knowledge Based","","","","","Secured back to designated fire box and highlight on upcoming toolbox and safety meeting.","2022-02-12T23:59:35","","Completed","2021-11-26T23:59:35","No","No","No","Internal"]
[null,null,null,22869,null,"123_1/12/2021 5:38:10 am","2021-11-20T23:59:35","Observation","Ship Staff","Ship Staff Insp.","INMARSAT-C Printer belt broke/tear off","Navigation - GMDSS & Communication","Communication","Equipment Related","","","","","NEWLY RECIEVED INMERSAT-C PRINTER INSTALLED AND TRIED OUT FOUND IN GOOD WORKING CONDITION.","2022-02-20T23:59:35","PELA210106","Completed","2022-01-03T23:59:35","No","No","No","Internal","spare parts has been connected to vessel on 02 Jan 2022, please update."]
[null,null,null,22864,null,"123_31/10/2021 9:26:57 pm","2021-11-24T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Few Fire Detectors found not operating properly","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","ALL FIRE DETECTORS TESTED AND TRIED OUT  CHANGED FAULTY FIRE DETECTOR. NOW ALL FIRE DETECTORS FOUND IN GOOD WORKING ORDER.","2022-02-24T23:59:35","PELA210076","Completed","2022-01-14T23:59:35","No","No","No","Internal","spare part will be connected to vessel at convenient port. pls monitor and update."]
[null,null,null,22894,null,"123_2/12/2021 10:33:52 pm","2021-11-24T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","No foot stopping arrangement in lathe and drilling machine. To raise requsition and install once receive","Miscellaneous","Safety / LSA / FFA","Knowledge Based","","","","","Recieved Foot switch connected to the syatem found working in good condition.","2022-02-24T23:59:35","","Completed","2022-02-15T23:59:35","No","No","No","Internal","pls advise RO reference number for tracking."]
[null,null,null,22895,null,"123_2/12/2021 10:55:44 pm","2021-11-24T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","One side of Galley hot plate out of order. Raise requisition of the requires spare","Accommodation","MLC Related","Equipment Related","","","","","DEFECTIVE HOTPLATE REPLACED WITH THE SPARE RECIEVED AND MADE OPERATIONAL.","2022-02-24T23:59:35","PELA210051","Completed","2022-01-16T23:59:35","No","No","No","Internal","Will connect to vessel at convenient port."]
[null,null,null,21113,null,"123_7/9/2021 11:34:43 am","2021-12-24T23:59:35","Defect","Ship Staff","Ship Staff Insp.","WBTS JFE Ballast Ace Unit not working due to failure on No. 2 TRO unit and Pneumatic Solenoid Valve Defective","Deck - Machinery","Cargo / Ballast Systems","Equipment Related","","","","","REPLACED FLOW CONTROL REGULATOR OF TRO UNIT NO.1 AND 2. UPDATED THE SYSTEM DATE REPLACED. REPLACED BUFFER SOLUTION AND TOTAL CHLORINE INDICATOR.","2022-02-27T23:59:35","PELA210102","Completed","2022-02-10T23:59:35","No","No","No","Internal","pls update latest working  condition."]
[null,null,null,23633,null,"123_14/1/2022 6:45:28 am","2022-01-09T23:59:35","Critical Equipment","Ship Staff","Ship Staff Insp.","Emergency generator no. 1 battery for starting  was defective due to the voltage drop. It need to be replace","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","EMERGENCY GENERATOR BATTERY BANK NO.1 REPLACED WITH THE RECIEVED BATTRIES AND TRIED OUT FOUND IN GOOD WORKING CONDITION.","2022-01-29T23:59:35","PELA220013 - EMERGENCY GENERATOR BATTERY","Completed","2022-01-16T23:59:35","No","No","No","Internal","will connect to vessel at ZHANGJIAGANG."]
[null,null,null,22893,null,"123_2/12/2021 10:16:02 pm","2022-01-28T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Isolated heavy rust in hydraulic line and air lines deck branches. Need to derust and paint","Deck - Pipe / Fittings","General Appearance","External Factors","","","","","Vessel has completed derusting all hydraulic, FW, fire and pneumatic lines on deck, apart from hydraulic pressure and return branch line for Hatch Cover operation. ","2022-05-30T23:59:35","","Completed","2022-05-28T23:59:35","No","No","No","Internal","pls speed up and advise date of completion."]
[null,null,null,24576,null,"123_2/2/2022 10:32:01 am","2022-01-29T23:59:35","Defect","Ship Staff","Ship Staff Insp.","ENGINE ROOM BLOWER AIR OPERATING PIPE FOR FLAPS FOUND RUSTED AND DETORIATED","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","REPLACED AIR PIPE FOR FLAP AND MADE OPERATIONAL.","2022-02-10T23:59:35","","Completed","2022-01-31T23:59:35","No","No","No","Internal"]
[null,null,null,22867,null,"123_31/10/2021 9:43:17 pm","2022-01-29T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Some Links of Hatch Cover Chain thin down & wasted","Deck - Machinery","Cargo / Ballast Systems","Equipment Related","","","","","Vessel has renewed the worn out chains of CH #1, # 3 , # 5, #6 , # 7. CH # 2 & # 4 derusted and coated. Hatch cover chains/connecting links recieved at Suez transit.","2022-04-28T23:59:35","PELA210022","Completed","2022-03-28T23:59:35","No","No","No","Internal","pls update here whether you have received it."]
[null,null,null,22868,null,"123_1/12/2021 10:38:36 pm","2022-01-29T23:59:35","Critical Equipment","Ship Staff","Ship Staff Insp.","broken gear teeth of bilge pump Main gear","E/R - Pumps","MARPOL Related","Equipment Related","","","","","VESSSEL CHANGED GEAR TEETH,CONNECTING ROD, PISTON RING AND PISTON NOW IN GOOD OPERATIONAL CONDITION.","2022-04-28T23:59:35","","Completed","2022-04-27T23:59:35","No","No","No","Internal","Pls  raise RO for spare parts as necessary."]
[null,null,null,24577,null,"123_15/2/2022 10:54:05 pm","2022-01-30T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Old refrigerator & Washing m/c are kept in laundry room, same to be disposed of at next convenient port.","Deck - Pipe / Fittings","General Appearance","Equipment Related","","","","","vessel oflanded the same at convinent port","2022-02-27T23:59:35","","Completed","2022-02-19T23:59:35","No","No","No","Internal"]
[null,null,null,24578,null,"123_15/2/2022 10:56:13 pm","2022-01-30T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Ballast water record book was found not filled properly as per required code, same to refill.","Documentation","Cert. & Docu.","Inappropriate Procedure","","","","","SAME WAS FILLED PROPERLY ","2022-02-27T23:59:35","","Completed","2022-02-19T23:59:35","No","No","No","Internal"]
[null,null,null,24566,null,"123_15/2/2022 10:33:02 pm","2022-01-30T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","vessel is installed with Daihatsu DG engine, as per instruction manual fuel pressure compensating regulator at inlet & outlet has to be changed every 12,000 hrs,if no records available of last change order for new regulator & replace on all 3 DGs.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","VESSEL REPLACED THE PRESSURE COMPENSATING REGULATOR AT INLET AND OUTLET FOR ALL 3 DG.","2022-05-30T23:59:35","PELA220039","Completed","2022-05-19T23:59:35","No","No","No","Internal","Spare part was ready, to supply onboard at convenient port"]
[null,null,null,24567,null,"123_15/2/2022 10:35:59 pm","2022-01-30T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Vessel has only one AHU & compressor, to keep as contingency back order compressor motor, One AHU blower complete & compressor sufficient spares for ohauling including shaft seal(alternatively can order for recon compressor)","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Vessel received the spare.","2022-06-14T23:59:35","PELA220031 & PELA220030","Completed","2022-07-03T23:59:35","No","No","No","Internal","will connect to vessel at convenient port."]
[null,null,null,24568,null,"123_15/2/2022 10:38:17 pm","2022-01-30T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","No oil level seen in the davit hyd system oil block tank, the block is covered with old denso tape so internal condition of block is unknown, SS to remove denso tape, check the condition of block & carry out buffing & fresh paint coating, then apply new denso tape.","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","vessel carried out maintenance, at present oil level can be seen.","2022-04-13T23:59:35","","Completed","2022-10-28T23:59:35","No","No","No","Internal","pls update latest status"]
[null,null,null,24569,null,"123_15/2/2022 10:40:34 pm","2022-01-30T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Set of hyd hoses for LB davit release device to be checked, raise RO fir required hoses if not available.","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","Grease tape from Life Boat and Rescue Boat removed and hose connections and couplings inspected. The same found to be in good condition. Grease tape renewed after inspection. ","2022-04-19T23:59:35","","Completed","2022-03-16T23:59:35","No","No","No","Internal","pls update latest status,"]
[null,null,null,24570,null,"123_15/2/2022 10:46:30 pm","2022-01-30T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Recent cargo hold & ballast tank inspection records to be made in company DNV form & uploaded in PAL.","Documentation","Cert. & Docu.","Inappropriate Procedure","","","","","Cargo Hold , Ballast Tank and Stool spaces inspection reports maintained in DNV form. Records kept onboard.","2022-04-18T23:59:35","","Completed","2022-04-18T23:59:35","No","No","No","Internal","pls update latest status."]
[null,null,null,24571,null,"123_15/2/2022 10:50:40 pm","2022-01-30T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Some hyd cylinder for hatch cover were found leaking, same to be rectified at first available opportunity","Deck - Machinery","General Appearance","Equipment Related","","","","","Vessel checked all hydraulic lifting jacks for leakages during operations . Leaking jacks overhauled and refitted, checked for leakages and found satisfactory. Vessel presently has 1  spare jack currently onboard.  Leaking hoses for hydraulic jacks renewed as required.","2022-04-09T23:59:35","PELA220034","Completed","2022-04-09T23:59:35","No","No","No","Internal","will connect to vessel at SUEZ, pls confirm receipt."]
[null,null,null,24572,null,"123_15/2/2022 10:44:33 pm","2022-01-30T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","PMS is not maintained properly, there are still 400 jobs to be triggered, PMS to be rectified as per briefing carried out","Documentation","Cert. & Docu.","Human Error","","","","","Jobs being triggered from PMS. Updation of maintenance being carried out at designated intervals.","2022-04-29T23:59:35","","Completed","2022-03-30T23:59:35","No","No","No","Internal","pls advise the date to  complete."]
[null,null,null,24573,null,"123_15/2/2022 10:20:09 pm","2022-01-30T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","All the heat exchanger/coolers which are SW cooled like aircon condenser, Atmospheric condenser, reefer etc. anodes have to be checked & replaced if required.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","VESSEL CHANGED THE ANODES FOR ALL THE SW COOLED EWUIPMENTS.","2022-02-23T23:59:35","","Completed","2022-03-06T23:59:35","No","No","No","Internal"]
[null,null,null,24574,null,"123_15/2/2022 10:25:02 pm","2022-01-30T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","luminance in steering room is very less ,same to be upgraded with LED lights","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","STEERING GEAR ROOM ALL LUMINANCE LIGHT UPGRADED TO LED.","2022-02-24T23:59:35","","Completed","2022-02-19T23:59:35","No","No","No","Internal"]
[null,null,null,24575,null,"123_15/2/2022 10:27:07 pm","2022-01-30T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","lathe m/c is not provided with protection glass on the check the prevent flying out of particles during cutting, same to be fabricated.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","VESSEL FABRICATED THE SAME FOR THE LATHE MACHINE","2022-02-23T23:59:35","","Completed","2022-02-20T23:59:35","No","No","No","Internal"]
[null,null,null,29305,67158,"123_Fri Mar 10 2023 13:44:09 GMT+0800","2022-02-27T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Nav Audit / Verification","Navigation Audit - VDR Playback software is not operational.","Navigation - VDR / BNWAS","Navigation","Equipment Related,External Factors","","","","","Navigation Audit - VDR Playback software found to be operational on further investigation.\nOfficers to be conversant with operation of VDR software. Master carried out VDR training with all officers.","2022-05-26T23:59:35","","Completed","2022-04-20T23:59:35","No","No","No","Internal"]
[null,null,null,29307,55119,"123_Fri Mar 10 2023 13:47:34 GMT+0800","2022-02-27T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Nav Audit / Verification","Navigation Audit - Master’s Standing instruction for ECDIS not posted on Bridge.","Navigation - ECDIS","Navigation","Human Error","","","","","Company procedure for master's standing orders for ECDIS posted on the bridge.","2022-05-26T23:59:35","","Completed","2022-04-21T23:59:35","No","No","No","Internal"]
[null,null,null,29308,18053,"123_Fri Mar 10 2023 13:55:04 GMT+0800","2022-02-27T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Nav Audit / Verification","Navigation Audit - Paper charts maintained in APCF have not been corrected since Aug 2021.","Navigation - Others","Navigation","External Factors","","","","","No Paper Chart corrections available onboard due to no contract with Auto Supply.","2022-05-26T23:59:35","","Completed","2022-04-21T23:59:35","No","No","No","Internal"]
[null,null,null,29309,59126,"123_Fri Mar 10 2023 13:57:05 GMT+0800","2022-02-27T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Nav Audit / Verification","Navigation Audit - Auto/Manual/NFU Steering change over procedures not posted on Bridge.","Navigation - Others","Navigation","Human Error","","","","","Steering change over procedures posted near the steering console for ease of operation during emergencies.","2022-05-26T23:59:35","","Completed","2022-04-21T23:59:35","No","No","No","Internal"]
[null,null,null,29310,15273,"123_Fri Mar 10 2023 13:59:17 GMT+0800","2022-02-27T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Nav Audit / Verification","Navigation Audit - Bridge equipment’s spares inventory not prepared.","Navigation - Others","Navigation","Behaviour Based,Human Error","","","","","Bridge equipment’s spares inventory updated and maintained.","2022-05-26T23:59:35","","Completed","2022-04-21T23:59:35","No","No","No","Internal"]
[null,null,null,29311,80108,"123_Fri Mar 10 2023 14:02:18 GMT+0800","2022-02-27T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Nav Audit / Verification","Navigation Audit – Notices to ensure ARPA Speed input is ‘Speed through water’ not posted on Radars.","Navigation - RADAR","Navigation","Human Error,Behaviour Based","","","","","Notices to ensure ARPA Speed input is ‘Speed through water’ posted on Radars.","2022-05-26T23:59:35","","Completed","2022-04-21T23:59:35","No","No","No","Internal"]
[null,null,null,29313,91557,"123_Fri Mar 10 2023 14:05:06 GMT+0800","2022-02-27T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Nav Audit / Verification","Navigation Audit - No shore acknowledgement received for GMDSS MF/HF DSC since 11 Dec 2021.","Navigation - GMDSS & Communication","Navigation","Human Error","","","","","GMDSS equipment tested with shore, received acknowledgement. The same kept for records.","2022-05-26T23:59:35","","Completed","2022-04-21T23:59:35","No","No","No","Internal"]
[null,null,null,29315,98879,"123_Fri Mar 10 2023 13:50:30 GMT+0800","2022-02-27T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Nav Audit / Verification","Navigation Audit - Forward foghorn not operational from Bridge.","Navigation - Others","Navigation","Equipment Related","","","","","Forward foghorn repairs carried and out and tested.","2022-05-26T23:59:35","","Completed","2022-04-21T23:59:35","No","No","No","Internal"]
[null,null,null,25912,13853,"123_Sat Jun 04 2022 02:31:11 GMT+0800","2022-04-13T23:59:35","Defect","Ship Staff","Ship Staff Insp.","BOILER SALINITY INDICATOR NOT WORKING","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","Old defective PCB was replaced with newly received spare and tried out found working in good condition.","2022-07-14T23:59:35","PELA220085","Completed","2022-07-04T23:59:35","No","No","No","Internal"]
[null,null,null,25915,76351,"123_Wed Jun 29 2022 17:33:31 GMT+0800","2022-04-25T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Post discharge operation in Gdansk, Poland it was observed that hatch cover access ladder railings and some steps are worn out and pose a threat of failure while accessing by shore personnel and ship's staff. On close inspection it was observed that steps have worn out with time.","Critical Equip.","Cargo / Ballast Systems","External Factors","","","","","Cargo Hold access steps and hand rails inspected and renewed at Dry Dock.","2023-11-16T23:59:35","","Completed","2023-10-20T23:59:35","Yes","No","No","Internal"]
[null,null,null,26958,null,"123_Thu Sep 22 2022 06:52:25 GMT+0000","2022-04-25T23:59:35","Non Conformity","PSC Insp.","PSC Inspection","ON BOARD TRANNING AND INSTRUCTION. (Code 17) Life Boat launching instruction without emergency lighting","","","","","","Life saving appliances","","","2022-07-25T23:59:35","","Completed","2022-05-24T23:59:35","No","No","No","External"]
[null,null,null,26959,null,"123_Thu Sep 22 2022 06:55:23 GMT+0000","2022-04-25T23:59:35","Non Conformity","PSC Insp.","PSC Inspection","BOILER FEED WATER SALINITY ALARM (Code 17) Boiler feed water salinity meter found switched off","E/R - Boiler","","","","","Alarms","","","2022-07-25T23:59:35","","Completed","2022-05-24T23:59:35","No","No","No","External"]
[null,null,null,26960,null,"123_Thu Sep 22 2022 06:58:08 GMT+0000","2022-04-25T23:59:35","Non Conformity","PSC Insp.","PSC Inspection","GUARDS - FENCING AROUND DANGEROUS MACHINERY PARTS (Code 10) Heavy steel pipe in the engine room not secured","","","","","","MLC, 2006","","","2022-07-25T23:59:35","","Completed","2022-05-24T23:59:35","No","No","No","External"]
[null,null,null,26961,null,"123_Thu Sep 22 2022 07:39:12 GMT+0000","2022-04-25T23:59:35","Non Conformity","PSC Insp.","PSC Inspection","PERSONEL EQUIPMENT FOR FIRE SAFETY (Code 10) The fire squad unable to establish communication by two-way portable radiotelephone apparatus","","Safety / LSA / FFA","","","","Fire safety","","","2022-07-25T23:59:35","","Completed","2022-05-24T23:59:35","No","No","No","External"]
[null,null,null,26962,null,"123_Thu Sep 22 2022 07:41:24 GMT+0000","2022-04-25T23:59:35","Non Conformity","PSC Insp.","PSC Inspection","OIL DISCH. MONITORING AND CONTROL SYSTEM (Code 17) Crew unable to show operational records in the memory of 15 ppm OWS before 24/04/2022 (calibration of OWS on the 02/06/2021)","","","","","","Pollution Prevention","","","2022-07-25T23:59:35","","Completed","2022-05-25T23:59:35","No","No","No","External"]
[null,null,null,25919,83824,"123_Thu May 26 2022 01:49:34 GMT+0800","2022-05-10T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","Port Side Accommodation ladder wire found damaged during routine greasing operation.","Deck - Machinery","Structural Condn. / WT integrity ","Equipment Related","","","","","Accommodation wire renewed with spare onboard. Requisition for 100% spare raised. ","2022-05-11T23:59:35","PELA220108","Completed","2022-05-11T23:59:35","No","No","No","Internal"]
[null,null,null,25913,44202,"123_Fri Jun 03 2022 23:42:34 GMT+0800","2022-05-14T23:59:35","Defect","Ship Staff","Ship Staff Insp.","In the process of surface preparation in accommodation it was observed that some steps in accommodation companionway (port & stbd) are completely worn out from underneath. The same was observed on steps on access to hatch cover top. \nThese steps need to be immediately cut and replaced to avoid injury to both ship's staff & shore personnel due to material failure. Vessel has raised requisition for checkered plate for cutting and renewing.","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","External Factors","","","","","Vessel received checkered plate in port call in Ghent, Belgium. Work in progress.","2022-09-29T23:59:35","PELA220108","Completed","2022-09-29T23:59:35","No","No","No","Internal"]
[null,null,null,25914,19755,"123_Fri Jun 03 2022 23:57:35 GMT+0800","2022-05-16T23:59:35","Observation","Ship Staff","Ship Staff Insp.","During derusting and coating of hydraulic lines on deck it was observed that branch line for hydraulics for hatch covers (pressure & return) have heavy rusting. On inspection it was found that outer dia. of pipe has reduced well below original, spares for renewal of pipes not available onboard. \nVessel to await receipt of spare pipes prior proceeding with derusting and coating of hydraulic branch lines.","Cargo Mach.","Cargo / Ballast Systems","External Factors","","","","","Poor condition hydraulic pipes were renewed at dry dock","2023-11-16T23:59:35","PELA220109","Completed","2023-10-21T23:59:35","Yes","No","No","Internal"]
[null,null,null,25920,78591,"123_Thu May 26 2022 04:30:47 GMT+0800","2022-05-24T23:59:35","Critical Equipment","Ship Staff","Ship Staff Insp.","Rescue Boat Davit Inboard Remote Control Wire found parted from the counterweight and Sheave Block all frozen. ","Deck - Machinery,LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","Replaced old wire with new onboard and raised requisition for the same, sheaves for remote control wire freed up, but required to renew. Requisition for the same raised. ","2022-05-25T23:59:35","PELA220111","Completed","2022-05-25T23:59:35","No","No","No","Internal"]
[null,null,null,29291,30781,"123_Thu Feb 23 2023 15:20:46 GMT+0800","2022-06-10T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Master's UPS was not working.","Elect. Mach. & Equip.","General Appearance","Equipment Related","","","","","Master’s cabin UPS received in Singapore on 21/01/2023.  Same renewed and tried out found working as per order. ","2023-02-28T23:59:35","PELA20119","Completed","2023-02-04T23:59:35","No","No","No","Internal"]
[null,null,null,25916,62429,"123_Wed Jun 29 2022 17:51:57 GMT+0800","2022-06-19T23:59:35","Critical Equipment","Ship Staff","Ship Staff Insp.","All mooring winches and windlass operating lever found frozen. Windlass lever found severely frozen to the extent of having to use a leverage handle to operate. A shore technician team was sent onboard to diagnose and rectify the problem, but the team were unable to do so due to time constraints and lack of spare parts.","Deck - Machinery","Mooring","Equipment Related","","","","","Vessel completed overhaul valves using o-ring kits supplied at Ghent. ","2022-08-30T23:59:35","PELA220123","Completed","2022-08-29T23:59:35","No","No","No","Internal"]
[null,null,null,25918,75264,"123_Thu Jun 30 2022 00:21:22 GMT+0800","2022-06-27T23:59:35","Critical Equipment,Observation","Ship Staff","Ship Staff Insp.","During anchoring operations for navigating to berth in Ghent, Belgium a leak was observed in the main fire line on deck, while running GS P/P for anchor wash. On closer inspection it was observed that the section of the pipe has rusted and holed from underneath.","Deck - Pipe / Fittings","Emgcy. Systems","External Factors","","","","","Soft patches applied and leak stopped as temporary repairs. Vessel presently discharging cargo in Ghent, Belgium and has voyage orders to load in Usta Luga  upon  completion. Fire line section to be cut and renewed at earliest opportunity with spares available onboard.","2022-08-30T23:59:35","","Completed","2022-08-13T23:59:35","No","No","No","Internal"]
[null,null,null,27996,48522,"123_Thu Oct 06 2022 11:01:30 GMT+0800","2022-06-27T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","Air motor for pilot access ladder port side (combination ladder) is not operational.","Deck - Machinery","ISM Related","External Factors,Equipment Related","","","","","Backlite sheet supplied and fabricated as per old size, fitted and tried out, working satisfactory, how ever speed is less, new motor will be ordered.","2022-10-10T23:59:35","","Completed","2022-11-22T23:59:35","No","No","No","Internal"]
[null,null,null,26664,75630,"123_Mon Aug 01 2022 05:51:55 GMT+0800","2022-07-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","PORT SIDE BUNKER DEVIT IN OPERATIONAL.","Deck - Machinery","Eng. / Strg. Comp.","Equipment Related","","","","","The motor was burnt in last year and vessel received new motor on 29th march 2022. Motor fitted in place but power converter for brake was wrong supplied. Original power converter input was 440VAC and supplied power converter input was 220VAC.After making wiring modification in panel and adjustment in brake, davit tried out with load and now its working as per order.\n\n","2022-09-29T23:59:35","","Completed","2022-09-01T23:59:35","No","No","No","Internal"]
[null,null,null,27102,52746,"123_Sun Sep 11 2022 16:22:32 GMT+0800","2022-07-12T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","Drinking water p/p motor no#1 and F.W hydrophore p/p no#1 was not working in auto due to faulty starter module ESM-1082A.","E/R - Aux. Mach.,Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","New spare modules found and replaced and then tried out now both p/p are working in auto.","2022-09-15T23:59:35","PELA220136","Completed","2022-09-07T23:59:35","No","No","No","Internal"]
[null,null,null,28122,18492,"123_Thu Oct 20 2022 17:06:53 GMT+0800","2022-08-04T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Drinking water p/p motor no#1 and F.W hydrophore p/p no#1 was not working in auto.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Due to faulty starter module ESM-1082A. New spare modules found and replaced and then tried out now both p/p are working in auto. ","2022-10-20T23:59:35","","Completed","2022-09-07T23:59:35","No","No","No","Internal"]
[null,null,null,27100,66238,"123_Sun Sep 11 2022 16:12:33 GMT+0800","2022-08-13T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Bridge telegraph printer pen was overlapping.","E/R - Main Engine","General Appearance","Equipment Related","","","","","Rectified by adjusting the roller and time date updated. Now working well. ","2022-08-20T23:59:35","","Completed","2022-08-18T23:59:35","No","No","No","Internal"]
[null,null,null,28126,21150,"123_Thu Oct 20 2022 16:38:06 GMT+0800","2022-08-20T23:59:35","Defect","Ship Staff","Ship Staff Insp.","ME JACKET CONTROLLER 3-WAY VALVE IS LEAKING FROM GLAND.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","spare received , same  has been used,  Main Engine HT Jacket controller 3-Way Valve Overhauled,  New Gland & O-rings renewed. leakage rectified on 14-Dec-2022","2022-12-20T23:59:35","","Completed","2022-12-14T23:59:35","No","No","No","Internal"]
[null,null,null,28004,10042,"123_Thu Oct 06 2022 09:41:09 GMT+0800","2022-08-21T23:59:35","Non Conformity,Defect","Ship Staff","Ship Staff Insp.","Provision store Weathertight door failed Light test.","","Safety / LSA / FFA","Inappropriate Procedure,Human Error,Knowledge Based","","","","","Channel of weathertight door derusted and rubber packing renewed, door handles freed. Light test passed.","2022-09-01T23:59:35","","Completed","2022-09-01T23:59:35","No","No","No","Internal"]
[null,null,null,27098,38202,"123_Thu Sep 08 2022 17:06:06 GMT+0800","2022-08-21T23:59:35","Defect","Ship Staff","Ship Staff Insp.","M.E HT Cooler seawater outlet pipe found leaking.","E/R - Main Engine,E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","During sailing, temporary repair been carried out since engine was running,\n AT port new pipe fabricated, Primer applied internally & fitted back.\nLeakage rectified","2022-09-09T23:59:35","","Completed","2022-09-06T23:59:35","No","No","No","Internal",""]
[null,null,null,27989,42438,"123_Thu Oct 06 2022 09:35:48 GMT+0800","2022-08-23T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Ship name on port and stbd side Bow have faded. and rust stain marks visible.","Hull & Tanks","General Appearance","External Factors","","","","","To derust and paint/stencil the ship name on port and stbd side Bow area at available anchorage with necessary permission from work overside from company and port. Vessel did not received permission from abbot point port authorities for carrying out overside work.Vsl will try to carry out work in upcoming anchorage in haldia.","2022-11-30T23:59:35","","Completed","2022-10-26T23:59:35","No","No","No","Internal"]
[null,null,null,28005,30623,"123_Thu Oct 06 2022 09:43:53 GMT+0800","2022-08-23T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Fwd stbd side 1 No fairlead not rotating freely and found frozen","Deck - Mooring Machinery","Mooring","External Factors,Human Error","","","","","fairlead dismantled, cover renewed, greased and fairlead moving freely now.","2022-09-30T23:59:35","","Completed","2022-09-27T23:59:35","No","No","No","Internal"]
[null,null,null,27988,32829,"123_Thu Oct 06 2022 09:21:07 GMT+0800","2022-08-25T23:59:35","Non Conformity","Ship Staff","Ship Staff Insp.","At various Locations on Main fire line doubler are observed to have been insterted.","","Safety / LSA / FFA","External Factors,Behaviour Based,Knowledge Based","","","","","Doubler sections to be renewed. Presently vsl have removed 4 section of pipe where doubler was insterted. at present there are 6 doubler present in main fire line.","2022-11-30T23:59:35","","Completed","2022-10-26T23:59:35","No","No","No","Internal"]
[null,null,null,28000,34548,"123_Thu Oct 06 2022 15:39:35 GMT+0800","2022-08-25T23:59:35","Defect","Ship Staff","Ship Staff Insp.","No.1 to No.6 hatch cover chain drive Sprocket have drop oil leakages.","Deck - Machinery","General Appearance","External Factors","","","","","Hatch cover oil leakages rectified by renewing o'rings.","2022-11-15T23:59:35","","Completed","2022-11-15T23:59:35","No","No","No","Internal"]
[null,null,null,28112,24332,"123_Thu Oct 20 2022 15:24:51 GMT+0800","2022-08-27T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Low insulation alarm coming from Galley. ","Elect. Mach. & Equip.","General Appearance","Equipment Related","","","","","Checked and found it is Hotplate no#3. New hot plate received. Renewed and then tried out now no low insulation alarm is coming from galley.","2023-02-08T23:59:35","PELA220171","Completed","2023-01-26T23:59:35","No","No","No","Internal"]
[null,null,null,27104,31790,"123_Thu Sep 15 2022 16:06:43 GMT+0800","2022-08-27T23:59:35","Non Conformity","Ship Staff","Ship Staff Insp.","Paint locker Sprinkler system valve found frozen and drain valve choked. Sprinker system found not operational","Deck - Pipe / Fittings,LSA / FFA","Safety / LSA / FFA","Inappropriate Procedure","","","","","Renewed Sprinker valve of paint store and drain valve cleared. sprinker system tried out found operational.","2022-09-16T23:59:35","","Completed","2022-09-03T23:59:35","No","No","No","Internal"]
[null,null,null,26666,80714,"123_Fri Sep 02 2022 12:45:58 GMT+0800","2022-08-28T23:59:35","Critical Equipment","Ship Staff","Ship Staff Insp.","Fire line have leakage between HC 6 and 7 , Fwd of No.7 and Abreast hatch cover No.7","Deck - Pipe / Fittings","Safety / LSA / FFA","External Factors","","","","","1 section renewed and other two section have be repaired. ","2022-09-09T23:59:35","","Completed","2022-09-29T23:59:35","No","No","No","Internal"]
[null,null,null,26667,64195,"123_Fri Sep 02 2022 12:40:11 GMT+0800","2022-08-30T23:59:35","Defect","Ship Staff","Ship Staff Insp.","hawser/Mooring winches and windlass brake lining have thinned down and most of them seem to have worn out.","Deck - Machinery","Mooring","Inappropriate Procedure,Equipment Related","","","","","De-rusting of Port side windlass drum & brake lining pad  renewed.\nDe-rusting of all mooring winches drum & brake lining pad  renewed.","2022-11-29T23:59:35","","Completed","2023-01-14T23:59:35","No","No","No","Internal"]
[null,null,null,28001,37179,"123_Thu Oct 06 2022 10:03:08 GMT+0800","2022-08-30T23:59:35","Defect","Ship Staff","Ship Staff Insp.","All Safety latches for provision crane, Bunker davit, General handling crane and  either missing or rusted or frozen or not spring loaded.","","","Inappropriate Procedure,Knowledge Based","","","","","Spring loaded safety latches installed on all cranes hooks.","2022-09-30T23:59:35","","Completed","2022-09-30T23:59:35","No","No","No","Internal"]
[null,null,null,28002,53343,"123_Thu Oct 06 2022 10:10:05 GMT+0800","2022-08-30T23:59:35","Non Conformity","Ship Staff","Ship Staff Insp.","Galley vent on B deck Broken from hinges, rubber packing wasted.","Accommodation","Safety / LSA / FFA","Inappropriate Procedure,External Factors","","","","","Door repaired and broken hinges fabricated new. rubber packing renewed.","2022-09-15T23:59:35","","Completed","2022-09-10T23:59:35","No","No","No","Internal"]
[null,null,null,27992,71066,"123_Thu Oct 06 2022 10:24:12 GMT+0800","2022-08-31T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Pilot Access ladder  (ACCOMODATION LADDER) motor emergency handle found frozen of port side and missing of stbd side.","","Emgcy. Systems","Equipment Related","","","","","derusted and greased the frozen handle and fabricate new handle for stbd side motor.","2022-10-15T23:59:35","","Completed",null,"No","No","No","Internal"]
[null,null,null,28120,54733,"123_Thu Oct 20 2022 16:43:40 GMT+0800","2022-09-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Low insulation alarm was coming from fwd insulation meter lighting panel.","Deck - Machinery","Cargo / Ballast Systems","Equipment Related","","","","","1S cargo light receptacle assembly with cable found burnt. New cable stripped out and new receptacle fitted. Now no low insulation is coming from fwd lighting","2022-09-07T23:59:35","","Completed","2022-09-02T23:59:35","No","No","No","Internal"]
[null,null,null,27099,46986,"123_Thu Sep 08 2022 17:13:09 GMT+0800","2022-09-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","GE Auto-backwash filter found leaky from Motor gland. ","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Filter assembly opened up,  all the candles removed, replaced with new cleaned one,  Motor gland X-ring renewed.  used spares are been updated in PAL also.\nLeakage rectified.","2022-09-15T23:59:35","","Completed","2022-09-07T23:59:35","No","No","No","Internal"]
[null,null,null,28124,29784,"123_Thu Oct 20 2022 17:14:33 GMT+0800","2022-09-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","2.\tAir conditioning compressor was not coming on 100% load (Running on 67% capacity). ","Accommodation","Crew Management","Equipment Related","","","","","Checked and found wrong wiring for SNS switch carried out same connected as per diagram and then tried out in auto now compressor is running on 100% capacity.","2022-09-30T23:59:35","","Completed","2022-09-19T23:59:35","No","No","No","Internal"]
[null,null,null,27101,48659,"123_Sun Sep 11 2022 16:18:26 GMT+0800","2022-09-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","220V, Low insulation alarm was coming in fwd insulation meter lighting panel.","Cargo Mach.,Elect. Mach. & Equip.","Cargo / Ballast Systems","Equipment Related","","","","","1S cargo light receptacle assembly with cable found burnt due to this, low insulation alarm was coming. New cable stripped out and new receptacle fitted. Now no low insulation is coming from fwd lighting. panel.","2022-09-04T23:59:35","","Completed","2022-09-02T23:59:35","No","No","No","Internal"]
[null,null,null,27991,71646,"123_Thu Oct 06 2022 10:21:20 GMT+0800","2022-09-02T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Emergency handle for Port and stbd gangway missing.","Deck - Machinery","Emgcy. Systems","Equipment Related","","","","","fabricated emg winch handles for port and stbd gangway.","2022-10-15T23:59:35","","Completed",null,"No","No","No","Internal"]
[null,null,null,28121,58110,"123_Thu Oct 20 2022 16:58:44 GMT+0800","2022-09-04T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Aux. boiler main burner was not firing in auto after pilot burner running.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","Checked and found the intensity of the fire was not able to read the flame eye and due to that burner tripped. Both flame eye cleaned. Flame detector relay found okay. FD fan flap found stuck and it was not closing when pilot burner fires. Flap freed up and flap coil contacts cleaned and tried out now main burner is firing in auto mode. ","2022-09-30T23:59:35","","Completed","2022-09-05T23:59:35","No","No","No","Internal"]
[null,null,null,27103,71685,"123_Sun Sep 11 2022 16:28:07 GMT+0800","2022-09-05T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","Aux. boiler main burner was not firing in auto after pilot burner running.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","Checked and found the intensity of the fire was not able to read the flame eye and due to that burner tripped. Both flame eye cleaned. Flame detector relay found okay. FD fan flap found stuck and it was not closing when pilot burner fires. Flap freed up and flap coil contacts cleaned and tried out now main burner is firing in auto mode.",null,"","Completed","2022-09-05T23:59:35","No","No","No","Internal"]
[null,null,null,28123,34438,"123_Thu Oct 20 2022 17:09:22 GMT+0800","2022-09-08T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Officer’s laundry dryer no#2 found not working. ","Accommodation,Elect. Mach. & Equip.","General Appearance","Equipment Related","","","","","Checked found plug burnt and rotary drum tight to turn. Burnt 3 pin plug renewed. Dryer opened up and adjustment carried out on the pulley side and then tried out now dryer working well.","2022-09-15T23:59:35","","Completed","2022-09-09T23:59:35","No","No","No","Internal"]
[null,null,null,27105,19933,"123_Sun Sep 11 2022 16:31:06 GMT+0800","2022-09-08T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Officer’s laundry dryer no#2 found not working.","Accommodation","General Appearance","Equipment Related","","","","","Checked found plug burnt and rotary drum tight to turn. Burnt 3 pin plug renewed. Dryer opened up and adjustment carried out on the pulley side and then tried out now dryer working well",null,"","Completed","2022-09-09T23:59:35","No","No","No","Internal"]
[null,null,null,27997,14179,"123_Thu Oct 06 2022 10:32:46 GMT+0800","2022-09-12T23:59:35","Defect","Ship Staff","Ship Staff Insp.","All mooring winches on forward deck, between hatch 1 and\n2, between hatch 6 and 7 and aft mooring deck, brake drum\nsurfaces are rusted and have uneven surfaces.","Deck - Mooring Machinery","Mooring","External Factors","","","","","Dismantled and renewed the SS surface of all Mooring winches.","2023-12-06T23:59:35","","Completed","2023-09-02T23:59:35","No","No","No","Internal"]
[null,null,null,27998,17267,"123_Thu Oct 06 2022 15:36:21 GMT+0800","2022-09-20T23:59:35","Non Conformity","Ship Staff","Ship Staff Insp.","Port and stbd draft marks and plimsol marks have rusted and faded.","Hull & Tanks","Cargo / Ballast Systems","External Factors","","","","","to derust and paint the plimsol marks and draft marks. Require port permission has same can be done only at anchorage and in ballast condition. In  abbot point vsl did not get permission to carry out work at anchorage.","2022-10-30T23:59:35","","Completed","2022-11-03T23:59:35","No","No","No","Internal"]
[null,null,null,27999,86445,"123_Thu Oct 06 2022 10:34:21 GMT+0800","2022-09-22T23:59:35","Non Conformity","Ship Staff","Ship Staff Insp.","Quick-acting cleats and crutches for cargo hold no. 1,3&4were found corroded and the rubber washers harden and painted.","Deck - Machinery","Structural Condn. / WT integrity ","Equipment Related","","","","","Paint removed and damaged rubber washer renewed 13 pcs in total.  of all hatches.","2022-10-20T23:59:35","","Completed",null,"No","No","No","Internal"]
[null,null,null,27987,12750,"123_Thu Oct 06 2022 09:14:57 GMT+0800","2022-09-28T23:59:35","Non Conformity","Ship Staff","Ship Staff Insp.","Section of fire main line abreast hatch No.6 found with minor drop leakages and also expansion joint found with drop leakage. also Some section between 5 and 6 require renewal.","Deck - Pipe / Fittings","Safety / LSA / FFA","External Factors","","","","","All leaking sections have been renewed.","2022-10-15T23:59:35","","Completed","2022-09-29T23:59:35","No","No","No","Internal"]
[null,null,null,27993,13219,"123_Thu Oct 06 2022 10:28:22 GMT+0800","2022-09-28T23:59:35","Non Conformity","Ship Staff","Ship Staff Insp.","Stbd side Bridge wing MOB lifebuoy found cracked during inspection.","LSA / FFA","Safety / LSA / FFA","External Factors","","","","","Received new lifebuoy at Singapore stenciled and  replace the damage with new one.\n","2022-10-20T23:59:35","","Completed","2023-01-23T23:59:35","No","No","No","Internal"]
[null,null,null,28003,16525,"123_Thu Oct 06 2022 10:26:16 GMT+0800","2022-09-30T23:59:35","Non Conformity","Ship Staff","Ship Staff Insp.","Grab line for Rescue boat found broken","LSA / FFA","Emgcy. Systems","Inappropriate Procedure","","","","","Renewed stbd side Rescue boat Grab line.",null,"","Completed","2022-09-30T23:59:35","No","No","No","Internal"]
[null,null,null,27994,16498,"123_Thu Oct 06 2022 10:40:33 GMT+0800","2022-10-01T23:59:35","Non Conformity","Ship Staff","Ship Staff Insp.","Quick acting cleats rubber washer of Hatch No 1 to 7 are not installed as per manufacture design","Deck - Machinery","Structural Condn. / WT integrity ","Equipment Related","","","","","installed all washer as per maker design.","2022-10-20T23:59:35","","Completed",null,"No","No","No","Internal"]
[null,null,null,28128,17391,"123_Thu Oct 20 2022 17:32:36 GMT+0800","2022-10-02T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Galley telephone is not working.","Miscellaneous","Communication","Equipment Related","","","","","Telephone headset received and same renewed. Now working well.","2022-11-30T23:59:35","PELA220207","Completed","2022-11-26T23:59:35","No","No","No","Internal"]
[null,null,null,27986,78721,"123_Wed Oct 05 2022 08:26:47 GMT+0800","2022-10-05T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Both Refrigeration plant Running hour meter not working","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","New Requisition PELA220190 created for new meters to install,, spares received and installed the same.\n","2022-11-30T23:59:35","","Completed","2022-10-17T23:59:35","No","No","No","Internal"]
[null,null,null,28110,96811,"123_Thu Oct 20 2022 17:22:18 GMT+0800","2022-10-05T23:59:35","Defect","Ship Staff","Ship Staff Insp.","ECDIS no#2 UPS was not coming on load after switching off the power supply. ","Elect. Mach. & Equip.,Navigation - ECDIS","Navigation","Equipment Related","","","","","UPS found defective same received and renewed. Now it's working as per order.","2023-02-14T23:59:35","PELA220201","Completed","2023-01-23T23:59:35","No","No","No","Internal"]
[null,null,null,28125,27258,"123_Thu Oct 20 2022 17:26:54 GMT+0800","2022-10-18T23:59:35","Critical Equipment","Ship Staff","Ship Staff Insp.","Rescue boat search light not working.","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","Same checked and found its toggle switch defective same replaced and tried out working well.  ","2022-10-18T23:59:35","","Completed","2022-10-18T23:59:35","No","No","No","Internal"]
[null,null,null,28113,71987,"123_Sat Dec 24 2022 19:18:37 GMT+0800","2022-10-21T23:59:35","Defect","Ship Staff","Ship Staff Insp.","440V low insulation coming from A/E#3 L.O priming p/p motor. ","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Requisition raised and after receiving the motor. Renewed and tried out. now no low insulation coming from A/E#3 L.O priming p/p motor.","2023-02-20T23:59:35","PELA220229","Completed","2023-01-24T23:59:35","No","No","No","Internal"]
[null,null,null,29300,54369,"123_Fri Mar 10 2023 13:04:27 GMT+0800","2022-10-23T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Nav Audit / Verification","Compass error not verified from 12 Oct to 17 Oct 2022.","Navigation - Others","Navigation","External Factors","","","","","Compass error was obtained by OOW upon clear sky during watch.\nLogged in Compass error log book and verified by Master.","2023-01-23T23:59:35","","Completed","2022-12-23T23:59:35","No","No","No","Internal"]
[null,null,null,29301,82624,"123_Fri Mar 10 2023 13:23:21 GMT+0800","2022-10-23T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Nav Audit / Verification","The blind sector for the S-band Radar is not posted next to the Radar.","Navigation - RADAR","Navigation","Behaviour Based,Human Error","","","","","The blind sector for the S-band Radar was misplaced somehow. \nSame was found and posted next to the Radar.","2023-01-23T23:59:35","","Completed","2022-10-26T23:59:35","No","No","No","Internal"]
[null,null,null,29302,95443,"123_Fri Mar 10 2023 13:26:12 GMT+0800","2022-10-23T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Nav Audit / Verification","Record for Auto/Hand steering changeover position not entered in bell book or deck logbook on departure port (Singapore).","Navigation - Others","Navigation","Human Error","","","","","Change of Auto/Hand steering was recorded with position, Time and date in bell book or Deck Log book.","2023-01-23T23:59:35","","Completed","2022-10-24T23:59:35","No","No","No","Internal"]
[null,null,null,29304,73775,"123_Fri Mar 10 2023 13:31:30 GMT+0800","2022-10-23T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Nav Audit / Verification","Time Hard-over to hard-over recorded as 27 seconds in the Pilot card was pre-printed.","Navigation - Others","Navigation","Human Error","","","","","On next arrival Port, After the steering test , Time duration for Hard over to Hard over was written/Recorded Manually on Pilot Card with Pen.","2023-01-23T23:59:35","","Completed","2022-10-27T23:59:35","No","No","No","Internal"]
[null,null,null,29312,18798,"123_Fri Mar 10 2023 13:28:56 GMT+0800","2022-10-23T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Nav Audit / Verification","One of the navigation lights  (RAM) on the Christmas tree was found out of order.","Navigation - Others","Navigation","Behaviour Based,Human Error","","","","","Navigation lights  (RAM) on the Christmas tree was replaced with new bulb by ETO. Made operational.","2023-01-23T23:59:35","","Completed","2022-10-24T23:59:35","No","No","No","Internal"]
[null,null,null,28129,58972,"123_Sat Dec 24 2022 23:41:04 GMT+0800","2022-10-26T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Bridge telegraph logger printer overwriting.","Elect. Mach. & Equip.","General Appearance","Equipment Related","","","","","Found its cartridge defective same ordered. New cartridge fitted in place and now no overwriting is happening.","2022-12-05T23:59:35","PELA220235","Completed","2022-11-26T23:59:35","No","No","No","Internal"]
[null,null,null,28131,85646,"123_Sat Dec 24 2022 23:48:33 GMT+0800","2022-10-31T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","BWTS VFD for chemical and neutralizer p/p showing error (E.PE2). Both ballasting and de-ballasting was not possible without non operational VFD.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","VFD ordered and same installed. Proper settings carried out by technician and tried out now VFD running as per order.","2022-11-15T23:59:35","PELA225038","Completed","2022-11-07T23:59:35","No","No","No","Internal"]
[null,null,null,28118,54004,"123_Mon Dec 26 2022 04:37:48 GMT+0800","2022-11-04T23:59:35","Defect","Ship Staff","Ship Staff Insp.","During routine overhauling of Hatch cover hydraulic pump Motor No.2, found spider of spider coupling broken, ROB is Nil, RO created for renewing broken spider. ","Elect. Mach. & Equip.","","Equipment Related","","","","","Item received and renewed and tried out now no abnormal sound is coming while starting and stopping the pump.","2023-02-03T23:59:35","PELA220234","Completed","2023-01-27T23:59:35","No","No","No","Internal"]
[null,null,null,28116,97675,"123_Sat Dec 24 2022 23:53:39 GMT+0800","2022-11-05T23:59:35","Defect","Ship Staff","Ship Staff Insp.","FBB 500 internet not working.","Elect. Mach. & Equip.","Communication","Equipment Related","","","","","FBB system discontinued from the ship and Iridium Certus system installed. System tried out found working as per order.","2023-02-04T23:59:35","PELA225040","Completed","2023-01-21T23:59:35","No","No","No","Internal"]
[null,null,null,28119,51746,"123_Mon Dec 26 2022 04:34:50 GMT+0800","2022-11-10T23:59:35","Defect","Ship Staff","Ship Staff Insp.","BWTS TRO unit no.2 optic assembly LED sensor light not working, need to be renewed.","Elect. Mach. & Equip.","","Equipment Related","","","","","BWTS TRO unit no 2 optic assembly replaced with new spare received and made operational.","2023-02-09T23:59:35","PELA220237","Completed","2023-02-09T23:59:35","No","No","No","Internal"]
[null,null,null,28133,50022,"123_Sat Dec 24 2022 23:57:23 GMT+0800","2022-11-17T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Fresh water p/p motor no#2 was not changing over to auto. ","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Checked found its PCB 1082A defective same renewed. Now it’s working well in both auto and manual mode",null,"","Completed","2022-11-18T23:59:35","No","No","No","Internal"]
[null,null,null,28115,52019,"123_Sat Dec 24 2022 19:58:17 GMT+0800","2022-11-18T23:59:35","Defect","Ship Staff","Ship Staff Insp."," UMS watch received alarm Fresh water Hydrophore No.1 Fresh water pump ABN STOP. Stby pump changed over and No.1 pump dismantled for inspection, found shaft broken, impeller eye key face sheared off from key way and electrical motor damaged, also casing mechanical seating area eccentrically worn out.\nAfter few hours of operation No.2 Pump lost suction, tried priming and was not taking suction  from double bottom center tank, pump dismantled for inspection, found impeller and casing ring in worn out condition, pump assembled back with new mechanical seal and mouth ring, pump running normal and its impeller need to be renewed as its cover end face have heavy scoring marks, it will cause imbalance the electrical motor.\n","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","","","","","Both fresh water pump made operational with new spares received.","2023-04-30T23:59:35","PELA220251 & PELA220250","Completed","2023-03-02T23:59:35","No","No","No","Internal"]
[null,null,null,28111,13645,"123_Sat Dec 24 2022 19:48:47 GMT+0800","2022-11-22T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Main Air compressor no: 2 found relief valve was lifting, Compressor isolated, water drained, opened up, found the Stages valves were remained opened with small pieces of metal, Piston opened up, found the piston gudgeon pin snap ring was missing & observed same was trapped in the valve plates, same overhauled, entire piston replaced with old used spare with new Piston rings, Con rod bearing & First stage valve.","E/R - Air Comp.","Emgcy. Systems","Equipment Related","","","","","New spares received and compressor made operational. ","2023-02-21T23:59:35","PELA220254","Completed","2023-02-13T23:59:35","No","No","No","Internal"]
[null,null,null,28114,52177,"123_Sat Dec 24 2022 19:54:11 GMT+0800","2022-11-22T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Boiler feed pump no: 2, found rattling sound observed during normal operation, pump isolated, opened up, found the Impeller liner plates are damaged & broken, All the stages impeller checked, found final stage impeller was damaged also, same overhauled & boxed back , Pump started no abnormal sound observed, but performance found deteriorated.\nOn 17 dec pump stopped due failure in operation and presently sailing with one boiler feed water pump and no spare.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","New multistage pump received, same installed in place. Suction and discharge line modified to adapt to new pump. Pump operation tried out and found in good working order.","2023-02-21T23:59:35","PELA220253","Completed","2023-02-16T23:59:35","No","No","No","Internal"]
[null,null,null,28130,22889,"123_Sun Dec 25 2022 00:00:41 GMT+0800","2022-11-30T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Hydro-blaster was tripping.","Deck - Machinery","General Appearance","Equipment Related","","","","","Checked and found main breaker cable loose same fitted back and tried out ampere checked found 31A (Rated ampere=56A). ","2022-12-01T23:59:35","","Completed","2022-11-30T23:59:35","No","No","No","Internal"]
[null,null,null,28132,22556,"123_Sun Dec 25 2022 00:05:08 GMT+0800","2022-12-01T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","FWG ejector p/p motor tripped. Insulation checked found zero. ","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Motor removed from place, dismantled and found winding bunt. Rotor shaft worn out.  Requisition raised for the motor. After receiving the motor on 17/12/2022, fitted in place, aligned with p/p and tried out found working well.","2022-12-20T23:59:35","PELA220255","Completed","2022-12-19T23:59:35","No","No","No","Internal"]
[null,null,null,28134,94083,"123_Mon Dec 26 2022 04:30:58 GMT+0800","2022-12-02T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Fresh water generator Ejector pump motor breaker tripped and 440 low insulation alarm received during UMS period. Motor insulation checked in place and found zero. Motor removed from place, dismantled for inspection found stator winding burnt, rotor drive end side bearing damaged and shaft worn out, bearing got damaged while running and its metal particles with grease stick to the stator winding lead to motor burning. Motor condition is  beyond repair and need to renew urgently to run Fresh water Generator. ","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","","","","","Requisition PELA220255 created in PAL, motor received at RIO GRANDE, fitted in place, running satisfactory.","2023-03-01T23:59:35","","Completed","2022-12-20T23:59:35","No","No","No","Internal"]
[null,null,null,28117,97176,"123_Sun Dec 25 2022 00:15:48 GMT+0800","2022-12-07T23:59:35","Defect","Ship Staff","Ship Staff Insp.","After actually getting the water low level in cascade tank found alarm was not received.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","New spare float received, same installed in place. Alarm found in good working order.","2023-03-06T23:59:35","Reference No : PELA220257","Completed","2023-02-02T23:59:35","No","No","No","Internal"]
[null,null,null,28127,92031,"123_Sat Dec 24 2022 19:10:10 GMT+0800","2022-12-11T23:59:35","Defect","Ship Staff","Ship Staff Insp.","440V low insulation alarm received from galley packaged A/C.","Accommodation","General Appearance","Equipment Related","","","","","Checked and found main power line cables rusty same rectified. ","2022-12-15T23:59:35","","Completed","2022-12-12T23:59:35","No","No","No","Internal"]
[null,null,null,29296,96402,"123_Fri Mar 10 2023 12:38:14 GMT+0800","2022-12-21T23:59:35","Observation","Ship Staff","Nav Audit / Verification","Course recorder paper to be signed by OOW after every watch.","Navigation - Others","Navigation","Behaviour Based","","","","","Course recorder paper to be signed by OOW after every watch.","2023-03-20T23:59:35","","Completed","2022-12-22T23:59:35","No","No","No","Internal"]
[null,null,null,29297,51939,"123_Fri Mar 10 2023 12:48:49 GMT+0800","2022-12-21T23:59:35","Observation","Ship Staff","Ship Staff Insp.","EGC Nav warnings / weather messages to be read, plotted and signed by all Navigating officers.","Navigation - GMDSS & Communication","Navigation","Human Error","","","","","Immediately All OOW read and Signed all navigation warnings/Weather message which was not read and signed.","2023-03-20T23:59:35","","Completed","2022-12-22T23:59:35","No","No","No","Internal"]
[null,null,null,29299,43112,"123_Fri Mar 10 2023 12:59:03 GMT+0800","2022-12-21T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Bridge walkie Talkies battery  found drained & should always be charged and spare charged battey to be kept along with.","Miscellaneous","Navigation","Behaviour Based,Human Error","","","","","Immediately drained battery  of walkie Talkie was replaced with Spare Battery. \nDrained battery was put in charge immediately for further use.","2023-03-20T23:59:35","","Completed","2022-12-24T23:59:35","No","No","No","Internal"]
[null,null,null,29306,38533,"123_Fri Mar 10 2023 12:54:39 GMT+0800","2022-12-21T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Compass/Gyro error to be verified at least once every watch.","Navigation - Others","Navigation","Human Error,Inappropriate Procedure","","","","","All OOW were instructed and briefed about verifying compass error at least once every watch.\nImmediately Compass error was verified.","2023-03-20T23:59:35","","Completed","2022-12-23T23:59:35","No","No","No","Internal"]
[null,null,null,29285,63318,"123_Fri Feb 24 2023 21:11:42 GMT+0800","2022-12-25T23:59:35","Observation","Ship Staff","Ship Staff Insp.","ER workshop drilling machine foot stop switch to be installed.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","ER workshop Drill machine Foot stop switch renewed and working properly.","2023-06-30T23:59:35","PELA230031","Completed","2023-08-21T23:59:35","No","No","No","Internal"]
[null,null,null,29289,33122,"123_Wed Feb 01 2023 10:23:45 GMT+0800","2023-01-10T23:59:35","Defect","Ship Staff","Ship Staff Insp.","ECDIS no#1 powered off instead of availability of main source. ","Navigation - ECDIS,Elect. Mach. & Equip.","Navigation","Equipment Related","","","","","UPS checked found not working as per order. Requisition raised. After receiving the UPS same renewed. Load test carried out now working as per order. ","2023-02-07T23:59:35","PELA230030","Completed","2023-01-23T23:59:35","No","No","No","Internal"]
[null,null,null,30128,28865,"123_Sun Apr 02 2023 01:11:51 GMT+0800","2023-01-21T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Vessel; has 4 nos of 20 ltrs foam for use with Applicators: No test records/ foam analysis reports available not delivery date records (if less than 3 years old)","LSA / FFA","Safety / LSA / FFA","Equipment Related,Inappropriate Procedure","","","","","Requisition has been raised for new foam solutions.\nREQUISITION NO: PELA230068 dated 20th Feb 2023","2023-05-31T23:59:35","REQUISITION NO: PELA230068 dated 20th Feb 2023","Completed","2023-04-30T23:59:35","No","No","No","Internal"]
[null,null,null,29287,29023,"123_Fri Mar 10 2023 12:12:55 GMT+0800","2023-01-22T23:59:35","Breakdown,Critical Equipment","Ship Staff","ISM Audit","Port side combination ladder air motor not operational.","Deck - Machinery","Emgcy. Systems","Equipment Related","","","","","Air motor was repaired by replacing blade made from Bakelite sheet but not operational. Requisition is raised for it awaiting for the supply.","2023-07-30T23:59:35","PELA230046","Completed","2023-07-25T23:59:35","No","No","No","Internal"]
[null,null,null,29298,34435,"123_Wed Feb 01 2023 10:34:44 GMT+0800","2023-01-22T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Boiler D.P transmitter was not maintaining the water level in the boiler. ","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","New DP transmitter received, installed and calibrated by shore technicians at Singapore on 08th Feb 2023. Operation of DP transmitter tested and same found in good working order.","2023-02-10T23:59:35","PELA230038","Completed","2023-02-07T23:59:35","No","No","No","Internal"]
[null,null,null,29294,88076,"123_Wed Feb 01 2023 10:40:52 GMT+0800","2023-01-28T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Fwd spring mooring winch control lever tight to hard to operate, while operating the handle broke down.","Deck - Mooring Machinery","Mooring","Equipment Related","","","","","Forward mooring winch operating block renewed with new spare and made operational.","2023-03-24T23:59:35","","Completed","2023-02-23T23:59:35","No","No","No","Internal"]
[null,null,null,29290,27940,"123_Thu Feb 23 2023 15:16:01 GMT+0800","2023-02-03T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","Deck air compressor motor tripped in overload safety. Megger test carried out found zero insulation. Motor disconnected, removed from place and dismantled in workshop. Found winding burnt.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Motor sent to workshop for rewinding in Singapore and after rewinding motor received and fitted in place and tried out found working as per order.","2023-02-15T23:59:35","PELA235011","Completed","2023-02-11T23:59:35","No","No","No","Internal"]
[null,null,null,29282,14733,"123_Thu Feb 23 2023 15:24:12 GMT+0800","2023-02-04T23:59:35","Defect","Ship Staff","Ship Staff Insp.","440V low insulation alarm is coming from galley hot plate no#2 and 4.","Accommodation,Elect. Mach. & Equip.","General Appearance","Equipment Related","","","","","After receiving the spares.  No#2 and 4 hot plate elements renewed and tried out now no low insulation is coming from galley cooling range.","2023-05-31T23:59:35","PELA230055","Completed","2023-05-09T23:59:35","No","No","No","Internal"]
[null,null,null,29288,95455,"123_Fri Mar 10 2023 12:02:53 GMT+0800","2023-02-07T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Control boxes for the hatch cover operating lever is wasted and not locking.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","Control boxes to cropped and renewed.","2023-08-02T23:59:35","","Completed","2023-07-17T23:59:35","No","No","No","Internal"]
[null,null,null,30130,36762,"123_Tue May 23 2023 00:39:43 GMT+0800","2023-02-12T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Foot stopper for drill machine in ER workshop was not available, to be installed.","E/R - Aux. Mach.","Safety / LSA / FFA","Inappropriate Procedure","","","","","Foot stopper installed after receiving spare and working satisfactorily.","2023-07-31T23:59:35","","Completed",null,"No","No","No","Internal"]
[null,null,null,30134,63227,"123_Mon May 22 2023 18:10:15 GMT+0800","2023-02-12T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Lifeboat davit name plate corroded.","LSA / FFA","General Appearance","Equipment Related","","","","","Lifeboat davit name plate to be greased to avoid corrosion","2023-03-12T23:59:35","","Completed","2023-03-10T23:59:35","No","No","No","Internal"]
[null,null,null,30136,72058,"123_Mon May 22 2023 18:27:40 GMT+0800","2023-02-12T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","valve handle at stbd side MGO bunker line rusted and slightly corroded.","Deck - Pipe / Fittings","General Appearance","Equipment Related","","","","","Valve handle at stbd side MGO bunker line rusted and slightly corroded, need to de-rust and paint.","2023-02-27T23:59:35","","Completed","2023-02-25T23:59:35","No","No","No","Internal"]
[null,null,null,30137,28823,"123_Mon May 22 2023 18:24:19 GMT+0800","2023-02-12T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Laundry room was mess and dirty through cleaning is required.","Accommodation","General Appearance","Behaviour Based","","","","","Laundry room was mess and dirty through cleaning is required to be carried out on regular basis and inspected.","2023-02-19T23:59:35","","Completed","2023-02-18T23:59:35","No","No","No","Internal"]
[null,null,null,30138,77317,"123_Mon May 22 2023 18:19:39 GMT+0800","2023-02-12T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Poop deck stbd side mooring winch hydraulic motor oil return pipe connection rusted and slightly corroded.","Deck - Machinery,Deck - Mooring Machinery","Mooring","Equipment Related","","","","","Poop deck stbd side mooring winch hydraulic motor oil return pipe connection rusted and slightly corroded. to de-rust and painting to be done.","2023-03-12T23:59:35","","Completed","2023-03-10T23:59:35","No","No","No","Internal"]
[null,null,null,30139,46966,"123_Mon May 22 2023 18:15:07 GMT+0800","2023-02-12T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Deck store is mess up.","Miscellaneous","General Appearance","Behaviour Based","","","","","Deck store to arrange and cleaned and maintain in order.","2023-02-27T23:59:35","","Completed","2023-02-24T23:59:35","No","No","No","Internal"]
[null,null,null,30142,36569,"123_Mon May 22 2023 23:24:18 GMT+0800","2023-02-12T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Anti-splash tape on ME unit2 and unit3 Fuel injection high pressure pipe connection missed out, need to wrap.","E/R - Main Engine","Eng. / Strg. Comp.","Inappropriate Procedure","","","","","Anti-splash tape wrapped on missing Fuel injection high pressure pipes and other required areas.","2023-02-22T23:59:35","","Completed","2023-02-14T23:59:35","No","No","No","Internal"]
[null,null,null,30143,31613,"123_Tue May 23 2023 00:36:13 GMT+0800","2023-02-12T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","220v panel low insulation meter shown at 0.5 M ohm, need to locate source of earthing and rectify.","Elect. Mach. & Equip.","Safety / LSA / FFA","Equipment Related","","","","","Found broken glass cover and water ingress in same. Renewed glass cover and rectified.","2023-02-19T23:59:35","","Completed","2023-02-17T23:59:35","No","No","No","Internal"]
[null,null,null,30144,61374,"123_Tue May 23 2023 00:43:26 GMT+0800","2023-02-12T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Engine room workshop need to be re-arranged in order.","Miscellaneous","Eng. / Strg. Comp.","Inappropriate Procedure","","","","","Engine room workshop area re-arranged.","2023-02-22T23:59:35","","Completed","2023-02-18T23:59:35","No","No","No","Internal"]
[null,null,null,30145,59774,"123_Tue May 23 2023 00:45:24 GMT+0800","2023-02-12T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Insulation mat was not available under welding machine in ER workshop. ","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Inappropriate Procedure","","","","","Insulation mat put for welding machine in ER workshop.","2023-02-19T23:59:35","","Completed","2023-02-18T23:59:35","No","No","No","Internal"]
[null,null,null,30146,45781,"123_Tue May 23 2023 00:47:08 GMT+0800","2023-02-12T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Steel pipe in steering gear room was not lashed properly.","Miscellaneous","Eng. / Strg. Comp.","Inappropriate Procedure","","","","","Same arranged and lashed to avoid falls.","2023-02-19T23:59:35","","Completed","2023-02-18T23:59:35","No","No","No","Internal"]
[null,null,null,30147,17057,"123_Tue May 23 2023 00:49:13 GMT+0800","2023-02-12T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Uncovered paint drum was found at corner of Engine Room, to be removed and put in paint store.","Miscellaneous","Eng. / Strg. Comp.","Inappropriate Procedure","","","","","All paint drums and buckets transferred to paint store.","2023-05-13T23:59:35","","Completed","2023-02-12T23:59:35","No","No","No","Internal"]
[null,null,null,29280,52600,"123_Mon Feb 20 2023 13:27:19 GMT+0800","2023-02-13T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Boiler both safety valve found leaking from valve seat. ","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","Overhauled boiler safety valve received at suez and installed at India anchorage.","2023-04-30T23:59:35","PELA 230050","Completed","2023-04-28T23:59:35","No","No","No","Internal"]
[null,null,null,29281,85779,"123_Mon Feb 20 2023 13:48:02 GMT+0800","2023-02-13T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Main air compressor No.2 overhauled on 13.02.2023 with old cylinder block as New spare could not be connected to vessel and compressor running with low efficiency. Old cylinder block in use has been re honed and have fine vertical grooves on high pressure side leading to air blow past.","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related","","","","","New cylinder block received, same installed and No 2 compressor made fully operational.","2023-03-30T23:59:35","PELA 220189 NGM supply.","Completed","2023-03-27T23:59:35","No","No","No","Internal"]
[null,null,null,29292,17921,"123_Thu Feb 23 2023 15:30:03 GMT+0800","2023-02-19T23:59:35","Critical Equipment","Ship Staff","Ship Staff Insp.","No#4 Cargo hold pre and main water ingress alarm came without water on the tip of the sensors. ","Critical Equip.,Cargo Mach.,Elect. Mach. & Equip.","Cargo / Ballast Systems","Equipment Related","","","","","Both sensors checked found water was ingresses due to leakage in manhole door. Both removed from place. New sensors fitted in place, connected and settings carried out as per maker manual. Tried out found working as per order.","2023-02-28T23:59:35","","Completed","2023-02-20T23:59:35","No","No","No","Internal"]
[null,null,null,29314,92736,"123_Mon Feb 20 2023 13:31:34 GMT+0800","2023-02-19T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Wax valve for Main air compressor cooling water system malfunctioning. Inlet water temperature to MAC observed to be 72 Deg cel, almost close to MAC outlet temperature of 76 Deg, where as operating range of thermostatic expansion valve is 38 deg cel to 49 deg cel.","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related","","","","","Remove thermostatic expansion valve and blank recirculation line. Connected FW cooling water inlet directly to MAC with fixed newly fabricated elbow/line. ","2023-03-31T23:59:35","PELA 230067 // PO cancelled (Not required)","Completed","2023-02-22T23:59:35","No","No","No","Internal"]
[null,null,null,29293,73788,"123_Thu Feb 23 2023 15:31:58 GMT+0800","2023-02-20T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","Master PC was not working. ","Elect. Mach. & Equip.","General Appearance","Equipment Related","","","","","New SSD installed as per office instructions and old M.2 SSD removed. Now master PC working as per order.","2023-02-28T23:59:35","","Completed","2023-02-21T23:59:35","No","No","No","Internal"]
[null,null,null,29283,33537,"123_Thu Feb 23 2023 15:35:33 GMT+0800","2023-02-21T23:59:35","Defect","Ship Staff","Ship Staff Insp.","ECDIS no#1, track ball was not working and ECDIS No#2 track ball is sluggish in operation.","Elect. Mach. & Equip.,Navigation - ECDIS","Navigation","Equipment Related","","","","","Both ECDIS Track ball renewed.","2023-07-31T23:59:35","PELA230069","Completed","2023-08-30T23:59:35","No","No","No","Internal"]
[null,null,null,29284,65854,"123_Thu Feb 23 2023 15:38:25 GMT+0800","2023-02-22T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","FWD talk back speaker found damaged and not in operational.","Elect. Mach. & Equip.","Communication","Equipment Related","","","","","Spares received and tried out found working as per order.","2023-05-30T23:59:35","PELA230072","Completed","2023-05-03T23:59:35","No","No","No","Internal"]
[null,null,null,29303,75866,"123_Fri Mar 10 2023 12:21:46 GMT+0800","2023-02-22T23:59:35","Observation,Defect","Ship Staff","Ship Staff Insp.","Provisions crane and bunker davit carne sheave found to be frozen.","Deck - Machinery","ISM Related","Equipment Related","","","","","blocks for the provision crane and bunker davit was dismantle, derusting and painting carried frozen pin freed.","2023-03-15T23:59:35","","Completed","2023-02-27T23:59:35","No","No","No","Internal"]
[null,null,null,29295,85118,"123_Wed Mar 01 2023 17:08:01 GMT+0800","2023-02-23T23:59:35","Defect","Ship Staff","Ship Staff Insp.","F.W Expansion tank low level alarm not received while trying out the alarm. ","E/R - Aux. Mach.,Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","Circuit checked found okay. Float removed from place by reducing the expansion tank water level. Float assembly cleaned, fitted back and tried out now alarm working as per order. ",null,"","Completed","2023-02-24T23:59:35","No","No","No","Internal"]
[null,null,null,29687,88101,"123_Wed Mar 15 2023 21:14:42 GMT+0800","2023-03-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Emergency light panel E1 breaker no#7 was tripping.","Elect. Mach. & Equip.","General Appearance","Equipment Related","","","","","Checked found aft mooring winch well glass light shorting same opened up and found water ingress in it. Water removed with dry cloths and connector renewed. Tried out found now breaker no#7 is not tripping. ","2023-03-06T23:59:35","","Completed","2023-03-02T23:59:35","No","No","No","Internal"]
[null,null,null,29685,70294,"123_Wed Mar 15 2023 21:17:37 GMT+0800","2023-03-05T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Port side ladder winch limit switch tested and found not working.","Deck - Machinery,Elect. Mach. & Equip.","General Appearance","Equipment Related","","","","","Same disconnected, removed from place and new limit switch fitted in place and tried out found working as per order. ","2023-03-15T23:59:35","","Completed","2023-03-10T23:59:35","No","No","No","Internal"]
[null,null,null,29286,73163,"123_Fri Mar 10 2023 11:58:49 GMT+0800","2023-03-08T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Air line valve on deck are leakings.","Deck - Pipe / Fittings","General Appearance","Equipment Related","","","","","All leaky air valves, overhauled and fitted back.","2023-05-08T23:59:35","","Completed","2023-05-15T23:59:35","No","No","No","Internal"]
[null,null,null,29316,40549,"123_Sat Mar 11 2023 17:35:25 GMT+0800","2023-03-10T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Bosun store 440V connection socket for Hydro blaster found burned out.","Elect. Mach. & Equip.","General Appearance","Equipment Related","","","","","New socket installed.","2023-03-31T23:59:35","","Completed","2023-03-10T23:59:35","No","No","No","Internal"]
[null,null,null,29686,50311,"123_Fri Mar 31 2023 22:00:05 GMT+0800","2023-03-16T23:59:35","Defect","Ship Staff","Ship Staff Insp.","L.O purifier no#1, pneumatic valve of 3-way feed valve was malfunctioning.","E/R - Purifier","Eng. / Strg. Comp.","Equipment Related","","","","","Same overhauled and solenoid valve replaced with old repaired solenoid valve. Now L.O purifier 3-way valve working as per order. ","2023-04-07T23:59:35","","Completed","2023-03-17T23:59:35","No","No","No","Internal"]
[null,null,null,29688,85544,"123_Fri Mar 31 2023 22:03:12 GMT+0800","2023-03-24T23:59:35","Defect","Ship Staff","Ship Staff Insp.","BWTS, TRO unit no#2 failure alarm occurred during de-ballasting. ","Elect. Mach. & Equip.,Cargo Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Checked found optic assembly defective. Defective assembly removed and new assembly fitted and tried out the system working as per order. ","2023-03-31T23:59:35","","Completed","2023-03-24T23:59:35","No","No","No","Internal"]
[null,null,null,29684,43369,"123_Fri Mar 31 2023 22:07:44 GMT+0800","2023-03-28T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Boiler cascade tank float switch was giving false low level alarm.","E/R - Boiler,Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","Boiler Cascade Tank Float Switch replaced with new one.","2023-08-21T23:59:35","PELA230083","Completed","2023-08-21T23:59:35","No","No","No","Internal"]
[null,null,null,30127,29443,"123_Sun Apr 02 2023 00:19:33 GMT+0800","2023-04-01T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Fwd STBD side windlass operating lever is very hard to operate, need to be overhauled. ","Deck - Mooring Machinery","Mooring","Equipment Related","","","","","Control lever to dismantled and overhauled, changed the damage O-ring. ","2023-07-30T23:59:35","","Completed","2023-10-17T23:59:35","No","No","No","Internal"]
[null,null,null,30150,87815,"123_Tue May 23 2023 01:04:28 GMT+0800","2023-04-01T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Air leakages in deck piping.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","","","","","Leaking sections renewed.","2023-05-15T23:59:35","","Completed","2023-05-10T23:59:35","No","No","No","Internal"]
[null,null,null,31344,71039,"123_Thu Jun 15 2023 01:11:29 GMT+0800","2023-04-06T23:59:35","Non Conformity","Ship Staff","Ship Staff Insp.","Galley vent on b deck broken from hinges, rubber packing wasted","Miscellaneous","Emgcy. Systems","Equipment Related","","","","","Galley broken vent hinges welded and rubber packing renewed.","2023-07-06T23:59:35","","Completed","2023-05-29T23:59:35","No","No","No","Internal"]
[null,null,null,31343,19235,"123_Thu Jun 15 2023 01:15:05 GMT+0800","2023-04-18T23:59:35","Defect","Ship Staff","Ship Staff Insp.","440V low insulation was coming from no.4 hot plate","Elect. Mach. & Equip.","General Appearance","Equipment Related","","","","","hot plate renewed","2023-06-18T23:59:35","","Completed","2023-05-26T23:59:35","No","No","No","Internal"]
[null,null,null,30131,30250,"123_Fri May 05 2023 18:13:54 GMT+0800","2023-04-23T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","BWTS disinfectant p/p chemicals flow was not matching target value.","Cargo Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Disinfectant pump cleaned as per maker's instructions and tried out found chemical flow is matching with target value.","2023-04-28T23:59:35","","Completed","2023-04-26T23:59:35","No","No","No","Internal"]
[null,null,null,30133,58247,"123_Fri May 05 2023 18:02:44 GMT+0800","2023-04-23T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","BWTS disinfectant pump motor was tripping while running for 2 minutes.","Cargo Mach.,Elect. Mach. & Equip.","Cargo / Ballast Systems","Equipment Related","","","","","Issue resolved by upgrading the settings in VFD inverter as per maker instructions. Pump tried out at different frequency now its nor tripping and drawing current is in limit.","2023-04-29T23:59:35","","Completed","2023-04-25T23:59:35","No","No","No","Internal"]
[null,null,null,30377,73562,"123_Sat Jun 03 2023 00:02:05 GMT+0800","2023-04-27T23:59:35","Critical Equipment","Ship Staff","Ship Staff Insp.","15 PPM OCM FOUND DEFECTIVE","Critical Equip.","MARPOL Related","Equipment Related","","","","","OLD OCM REPLACED WITH NEW RECEIVED 15PPM OCM. WORKING IN GOOD ORDER.",null,"","Completed","2023-05-24T23:59:35","No","No","No","Internal"]
[null,null,null,30129,31548,"123_Thu May 18 2023 20:41:42 GMT+0800","2023-05-04T23:59:35","Defect","Ship Staff","Ship Staff Insp.","X-Band radar VRM switch is operational with some glitch. ","Navigation - Others,Critical Equip.","Navigation","Equipment Related","","","","","Radar Newly received keyboard installed, now VRM switch is working properly.","2023-08-10T23:59:35","PELA230118","Completed","2023-08-10T23:59:35","No","No","No","Internal"]
[null,null,null,30375,69244,"123_Fri Jun 02 2023 15:25:18 GMT+0800","2023-05-05T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Galley vent flap hinges wasted and broken","Accommodation","General Appearance","Equipment Related","","","","","To repair the hinges and fix back.","2023-05-31T23:59:35","","Completed","2023-05-25T23:59:35","No","No","No","Internal"]
[null,null,null,30132,79866,"123_Thu May 18 2023 14:57:40 GMT+0800","2023-05-05T23:59:35","Observation","Ship Staff","Ship Staff Insp.","ME FO high pressure pipes  locking nut both injector side and pump side for all units found loose during routine inspection.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","ME FO high pressure pipes  locking nut both injector side and pump side for all units found loose during routine inspection. All units locking nuts tightened as per makers recommendation and frequency for inspection by ships staff have been increased to avoid any catastrophic future incidents. Further to this all high pressure pipes will be loosened and retightened again with thread lock at first available port opportunity as above mentioned cant be done during incident as vessel was sailing and enroute.","2023-05-06T23:59:35","","Completed","2023-05-05T23:59:35","No","No","No","Internal"]
[null,null,null,30135,36087,"123_Fri May 05 2023 18:05:52 GMT+0800","2023-05-05T23:59:35","Defect","Ship Staff","Ship Staff Insp.","H.F.O Purifier no#1 motor was making abnormal noise.","E/R - Purifier,Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","Noise was coming from bearings. Motor dismantled and both bearings renewed and then boxed back and tried out found working as per order.","2023-05-06T23:59:35","","Completed","2023-05-05T23:59:35","No","No","No","Internal"]
[null,null,null,30149,33266,"123_Tue May 23 2023 01:08:06 GMT+0800","2023-05-05T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Found oil leakage through worn out filling plug of Hatch cover hydraulic ram.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","Plug renewed and leakage rectified.","2023-05-12T23:59:35","","Completed","2023-05-10T23:59:35","No","No","No","Internal"]
[null,null,null,30140,65187,"123_Mon May 22 2023 18:37:25 GMT+0800","2023-05-06T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Hose test of the hatch cover carried out found leaking","Cargo Mach.","Structural Condn. / WT integrity ","Equipment Related","","","","","Hose test of the hatch cover carried out found leaking, to do the welding of shimp plate on the FY-stoppers to increase the compression of the rubber packing. ","2023-05-20T23:59:35","","Completed","2023-05-11T23:59:35","No","No","No","Internal"]
[null,null,null,30141,18893,"123_Thu May 18 2023 20:32:45 GMT+0800","2023-05-08T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Aft bilge alarm was not coming.","E/R - Aux. Mach.,Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","Same removed from place and found float stuck due to mud same cleaned and then tried out found working well. ","2023-05-10T23:59:35","","Completed","2023-05-09T23:59:35","No","No","No","Internal"]
[null,null,null,30148,43428,"123_Tue May 23 2023 00:59:39 GMT+0800","2023-05-09T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Observed abnormal vibration and sound from HFO purifier no.1.","E/R - Purifier","Eng. / Strg. Comp.","Equipment Related","","","","","Complete vertical and horizontal shaft overhauled, renewed all consumable spares. Presently satisfactory.","2023-05-13T23:59:35","","Completed","2023-05-12T23:59:35","No","No","No","Internal"]
[null,null,null,30373,81941,"123_Fri Jun 02 2023 23:58:36 GMT+0800","2023-05-15T23:59:35","Defect","Ship Staff","Ship Staff Insp.","BANWAS ALARM NOT GETTING ACTIVATED IN SHIP'S OFFICE, CAPTAIN CABIN AND THIRD OFFICER CABIN.","Navigation - VDR / BNWAS","Safety / LSA / FFA","Equipment Related","","","","","NEW BNWAS PANEL UNIT INSTALLED BY SHORE TECHNICIANS. NOW BNWAS IS FULLY OPERATIONAL AND ACTVATED IN ALL LOCATIONS","2023-10-22T23:59:35","","Completed","2023-10-21T23:59:35","No","No","No","Internal"]
[null,null,null,30374,76891,"123_Sat Jun 03 2023 18:00:25 GMT+0800","2023-05-16T23:59:35","Defect,Observation","Ship Staff","Ship Staff Insp.","Ballast tank Air vent head rubber packing missing. ","Hull & Tanks","Cargo / Ballast Systems","Equipment Related","","","","","Rubber packing renewed","2023-08-15T23:59:35","","Completed","2023-10-20T23:59:35","No","No","No","Internal"]
[null,null,null,30372,58558,"123_Fri Jun 02 2023 15:33:46 GMT+0800","2023-06-01T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Save-alls dip tray to be fabricated below the control lever  of the hatch covers and  the hydraulic jacks to retain the oil in case of oil leakages.","Cargo Mach.","MARPOL Related","Industry Issue","","","","","To be carried out during ballast passage or dry dock.","2023-12-31T23:59:35","","Completed","2023-12-12T23:59:35","Yes","No","No","Internal"]
[null,null,null,30376,17004,"123_Sat Jun 03 2023 00:06:09 GMT+0800","2023-06-02T23:59:35","Observation","Ship Staff","Ship Staff Insp.","1 NO. FIRE HYDRANT FOUND LEAKING IN E/R BOTTOM PLATFORM.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","HYDRANT REMOVED FOR OVERHAULING. LAPPED AND TESTED FOR NO LEAKAGE.",null,"","Completed","2023-06-02T23:59:35","No","No","No","Internal"]
[null,null,null,32373,33686,"123_Thu Jun 15 2023 20:33:06 GMT+0800","2023-06-13T23:59:35","Defect","Ship Staff","Ship Staff Insp.","chiller unit coolant hose found leaking.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Chiller unit hose replaced ","2023-07-20T23:59:35","PELA230131","Completed","2023-10-20T23:59:35","No","No","No","Internal"]
[null,null,null,32372,14439,"123_Fri Jun 16 2023 15:54:46 GMT+0800","2023-06-16T23:59:35","Defect","Ship Staff","Mooring Audit","TOP PLATE OF PEDESTAL ROLLER ON AFT STATION FOUND HOLES & DAMAGED.","Miscellaneous","Mooring","Equipment Related","","","","","NEED TO RENEW OR FABRICATE NEW PLATES TO CHANGE THE DAMAGED ONE.","2023-07-23T23:59:35","","Completed","2023-06-30T23:59:35","No","No","No","Internal"]
[null,null,null,27095,54461,"123_Thu Sep 15 2022 14:18:48 GMT+0800","2023-07-02T23:59:35","Non Conformity","Ship Staff","Ship Staff Insp.","Fwd emergency light switch for Liferaft found not operational when tested with emg light kept in forecastle store","LSA / FFA","Emgcy. Systems","Inappropriate Procedure","","","","","Rectified  emergency light switch and operational.","2023-10-02T23:59:35","","Completed","2023-10-05T23:59:35","No","No","No","Internal","Trust this job has already been completed, kindly update 7 close out in DDRL."]
[null,null,null,27984,43718,"123_Thu Oct 06 2022 09:10:47 GMT+0800","2023-07-03T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Bridge Floor at various locations have been wasted or broken and Floor is uneven due to wasting of matting. Rubber matting was in place to cover the same.","Miscellaneous","General Appearance","External Factors","","","","","Renewed bridge floor by yard party at dry dock.","2023-10-03T23:59:35","","Completed","2023-09-25T23:59:35","No","No","No","Internal"]
[null,null,null,27985,40713,"123_Wed Oct 05 2022 08:30:00 GMT+0800","2023-07-05T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Fish room door heater missing, causing ice formation on door.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","Installed new heater on door at dry dock.","2023-10-05T23:59:35","PELA220191","Completed","2023-09-16T23:59:35","No","No","No","Internal"]
[null,null,null,29279,26488,"123_Mon Feb 20 2023 13:40:28 GMT+0800","2023-07-05T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Stern tube seals #1,2,3 found leaking leading to water ingress and oil outgress to and from gravity tank at varying draft conditions.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Forward and aft seal renewed at dry dock","2023-10-30T23:59:35","","Completed","2023-09-10T23:59:35","No","No","No","Internal"]
[null,null,null,27990,32394,"123_Thu Oct 06 2022 09:54:35 GMT+0800","2023-07-06T23:59:35","Non Conformity,Critical Equipment,Other","Ship Staff","Ship Staff Insp.","Emg generator room Natural vent cover missing.","LSA / FFA,Accommodation","Safety / LSA / FFA","Human Error,External Factors,Inappropriate Procedure","","","","","Emergency generator natural vent cover fabricated and installed.","2023-10-06T23:59:35","","Completed","2023-09-30T23:59:35","No","No","No","Internal","Long pending defect, kindly get this repair & close out in DDRL."]
[null,null,null,27090,78684,"123_Wed Sep 14 2022 19:05:15 GMT+0800","2023-07-06T23:59:35","Non Conformity","Ship Staff","Ship Staff Insp.","Galley vent on B deck Broken from hinges, rubber packing wasted.","Miscellaneous","Emgcy. Systems","Equipment Related","","","","","Fabricated & welded galley vent and renewed rubber packing.","2023-10-06T23:59:35","","Completed","2023-09-30T23:59:35","No","No","No","Internal","Kinddly get this galley vent fabricated on B deck & close in DDRL upon completion."]
[null,null,null,27088,22946,"123_Sun Sep 11 2022 16:06:03 GMT+0800","2023-07-18T23:59:35","Defect","Ship Staff","Ship Staff Insp.","440V low insulation was coming from no#4 hot plate.","Elect. Mach. & Equip.","General Appearance","Equipment Related","","","","","No. 2 and No. 4 hot plates elements were renewed after receiving spares. Now no low insulation alarm.","2023-10-18T23:59:35","PELA220171","Completed","2023-07-18T23:59:35","No","No","No","Internal","Already connected to vessel, please check & close out DDRL accordingly."]
[null,null,null,26665,25974,"123_Mon Aug 01 2022 13:47:19 GMT+0800","2023-07-19T23:59:35","Defect","Ship Staff","Ship Staff Insp.","During anchoring at Ust-luga, Russia outer roads deep water anchorage (UKC about 70 mtrs), vessel was walking back Port anchor up to 9 shackle in water. Before 9th shackle, the anchor chain was found to be twisted and kinked very badly, and not able to come out from the Spurling pipe. Some attempt was made to lower it but with no result. Ship staff managed to heave up Port anchor\nand vessel re-anchored safely using Starboard anchor.\n\nPresently, vessel can use Port anchor only up to 8 shackles, as beyond that the anchor chain is badly twisted and kinked.","Deck - Mooring Machinery","Mooring","External Factors","","","","","Rectified by yard party at dry dock.","2023-10-30T23:59:35","PELA220139","Completed","2023-09-05T23:59:35","No","No","No","Internal"]
[null,null,null,25917,93189,"123_Wed Jun 29 2022 18:00:39 GMT+0800","2023-07-21T23:59:35","Breakdown,Observation","Ship Staff","Ship Staff Insp.","Chain Locker pipe for leading anchor chain on deck under gypsie to spurling pipe in chain locker found rusted/wastage and holed.","Deck - Pipe / Fittings","General Appearance","External Factors","","","","","Cut and renewed by yard party at dry dock.","2023-10-17T23:59:35","","Completed","2023-08-28T23:59:35","Yes","No","No","Internal"]
[null,null,null,27096,63835,"123_Thu Sep 15 2022 16:03:13 GMT+0800","2023-07-24T23:59:35","Non Conformity","Ship Staff","Ship Staff Insp.","Provision store Weathertight door failed Light test.","","Structural Condn. / WT integrity ","Inappropriate Procedure","","","","","Derusted the retaining Channel of the rubber packing and renewed the rubber gasket as required.","2023-10-24T23:59:35","","Completed","2023-09-20T23:59:35","No","No","No","Internal","This is long pending job, kindly complete this job & update DDRL."]
[null,null,null,27995,10605,"123_Thu Oct 06 2022 15:32:35 GMT+0800","2023-07-25T23:59:35","Non Conformity","Ship Staff","Ship Staff Insp.","Fwd and aft port and Stbd Draft marks are faded.","Miscellaneous","Structural Condn. / WT integrity ","External Factors","","","","","Painted the draft marks at dry dock.","2023-10-25T23:59:35","","Completed","2023-09-03T23:59:35","No","No","No","Internal"]
[null,null,null,27094,36390,"123_Thu Sep 15 2022 14:15:46 GMT+0800","2023-07-25T23:59:35","Defect","Ship Staff","Ship Staff Insp.","All Safety latches for provision crane, Bunker davit, General handling crane and lifeboat hooks either missing or rusted or frozen or not spring loaded.","Deck - Machinery","Safety / LSA / FFA","External Factors","","","","","Renewed the safety latches and raised requisition & rectified the same.","2023-10-25T23:59:35","","Completed","2023-09-30T23:59:35","No","No","No","Internal","This job should have completed & DDRL to be closed accordingly."]
[null,null,null,27087,13407,"123_Wed Sep 14 2022 18:58:18 GMT+0800","2023-07-28T23:59:35","Observation","Ship Staff","Ship Staff Insp.","PILOT ACCESS LADDER (ACCOMODATION LADDER) MOTOR FOR PORT SIDE EMERGENCY HANDLE FROZEN AND STBD SIDE  HANDLE MISSING.","Deck - Machinery","Emgcy. Systems","Equipment Related","","","","","Dismantled the frozen handle and fabricated new handle.","2023-10-28T23:59:35","","Completed","2023-10-19T23:59:35","No","No","No","Internal","This job should have completed & DDRL updated accordingly."]
[null,null,null,27089,59944,"123_Wed Sep 14 2022 19:00:34 GMT+0800","2023-07-28T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Port and stbd gangway motor emergency handle missing.","Deck - Machinery","Emgcy. Systems","Equipment Related","","","","","Fabricated new emergency handle.","2023-10-28T23:59:35","","Completed","2023-10-10T23:59:35","No","No","No","Internal"]
[null,null,null,27091,15369,"123_Wed Sep 14 2022 19:08:38 GMT+0800","2023-07-28T23:59:35","Defect","Ship Staff","Ship Staff Insp.","forecastle deck Stbd side 1 No. fairlead found frozen","Deck - Mooring Machinery","Mooring","Equipment Related","","","","","Fair lead dismantled, cover renewed, gresed , fairlead moving freely now.","2023-10-28T23:59:35","","Completed","2023-09-27T23:59:35","No","No","No","Internal","Trust this job has already been completed, kindly check & update accordingly."]
[null,null,null,27092,65730,"123_Thu Sep 15 2022 14:08:37 GMT+0800","2023-07-28T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Aft tank Stbd side vent head rubber gasket sealing lip found damage on inspection.","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","External Factors","","","",""," Cropped and renewed the lip and  vent head renewed at dry dock.","2023-10-28T23:59:35","","Completed","2023-09-30T23:59:35","No","No","No","Internal","Please check & get the job completed asap."]
[null,null,null,27093,20941,"123_Thu Sep 15 2022 14:12:02 GMT+0800","2023-07-28T23:59:35","Defect","Ship Staff","Ship Staff Insp.","All mooring winches and windlass break band holding bolt have excessive gap and all found frozen.","Deck - Mooring Machinery","Mooring","Inappropriate Procedure","","","","","All mooring winches and windlass break band holding bolteased up and gap adjusted.","2023-10-28T23:59:35","","Completed","2023-09-28T23:59:35","No","No","No","Internal","This is long pending job, kindly complete asap"]
[null,null,null,27097,39864,"123_Fri Sep 16 2022 15:26:53 GMT+0800","2023-07-28T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Ship name on port and stbd side Bow have faded.","Hull & Tanks","General Appearance","External Factors","","","","","Job completed at dry dock.","2023-10-28T23:59:35","","Completed","2023-10-26T23:59:35","No","No","No","Internal","Vessel to take permission of port authority & office approval for the job. Please plan the job accordingly. This is long pending job & need to be completed asap."]
[null,null,null,32710,33943,"123_Wed Nov 15 2023 19:19:26 GMT+0800","2023-11-02T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","All hatch cover hyd control blocks to be derusted & Emg. Connection to be marked.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","","","","","Derusting of hatch cover control lever blocks & remarking of Emg. connection coupling ","2023-12-31T23:59:35","","Completed","2023-11-16T23:59:35","No","No","No","Internal"]
[null,null,null,32711,99848,"0_Wed Nov 15 2023 15:49:10 GMT+0800","2023-11-02T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","All ER stores & Workshop store to remove all the items & take inventory & secure them back properly","Miscellaneous","Eng. / Strg. Comp.","External Factors","","","","","ER store all, items removed, inventory taken. A new shell fabricated and fitted near AE platform (stbd. side) to accommodate AE and compressor spares. Updating inventory in PAL completed.","2023-12-31T23:59:35","","Completed","2023-12-05T23:59:35","No","No","No","Internal"]
[null,null,null,32712,29335,"0_Wed Nov 15 2023 16:14:27 GMT+0800","2023-11-02T23:59:35","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","No.1 FW hydrophore pp to be Fitted with new received spare & try out the system. New complete hydrophore pp to be fitted as well on base & electrical modification to be carried out, RO to be raised for electrical parts & other allied things.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","","","","","No. 1 FW hydrophore pump overhauled and fitted with new impeller and mechanical seal. The pump currently is in use with satisfactory performance. New hydrophore pump with self primer fitted in place after fabricating the base. The modification of pipelines and valves carried out. This pump is operational. ","2024-02-02T23:59:35","PELA235120","Completed","2024-01-01T23:59:35","No","No","No","Internal"]
[null,null,null,32713,36340,"0_Wed Nov 15 2023 16:25:57 GMT+0800","2023-11-02T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Some thermometers & Pressure gauges in ER show faulty reading & broken, same to be replaced with new spares, Month end checklist to be updated accordingly.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Faulty thermometers and pressure gauges in engine room replaced with new spare.","2024-01-30T23:59:35","","Completed","2024-01-03T23:59:35","No","No","No","Internal"]
[null,null,null,32714,11489,"0_Wed Nov 15 2023 16:28:51 GMT+0800","2023-11-02T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","All the Dry dock jobs carried out on deck & Engine side to be updated in PMS as applicable.","Documentation","Cert. & Docu.","External Factors","","","","","Updating of all jobs carried out during Dry dock in PMS is Done","2023-12-31T23:59:35","","Completed","2023-11-30T23:59:35","No","No","No","Internal"]
[null,null,null,32715,40103,"123_Wed Nov 15 2023 19:51:58 GMT+0800","2023-11-02T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","All Deck stores items to be removed, inventory to be taken & store properly back","Miscellaneous","General Appearance","External Factors","","","","","Rearrange & take proper inventory of all deck stores.","2023-12-02T23:59:35","","Completed","2023-11-03T23:59:35","No","No","No","Internal"]
[null,null,null,32716,18413,"123_Wed Nov 15 2023 19:53:46 GMT+0800","2023-11-02T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Forecastle store items inventory to be taken & secured properly.","Miscellaneous","Crew Management","External Factors","","","","","Rearrange & take proper inventory of forecastle store.","2023-12-02T23:59:35","","Completed","2023-11-14T23:59:35","No","No","No","Internal"]
[null,null,null,32717,84983,"123_Wed Nov 15 2023 19:57:43 GMT+0800","2023-11-02T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","No. of Max person allowed & load test with date to be marked on MOT ladder.","Deck - Pipe / Fittings","Safety / LSA / FFA","External Factors","","","","","Stenciling & marking of MOT ladder  max allowable person & load test.","2023-11-17T23:59:35","","Completed","2023-11-20T23:59:35","No","No","No","Internal"]
[null,null,null,32718,26661,"123_Wed Nov 15 2023 20:32:15 GMT+0800","2023-11-02T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Port Side Fuel oil tank Vent cover opening to be extended to the bottom.","Deck - Pipe / Fittings","MARPOL Related","External Factors","","","","","Fabricated & installed  port side fuel oil tank vent cover.","2024-02-15T23:59:35","","Completed","2024-01-22T23:59:35","No","No","No","Internal"]
[null,null,null,32719,33745,"123_Wed Nov 15 2023 19:36:59 GMT+0800","2023-11-02T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","30 Washers of the cleats to be fully prepared & bent washers to be replaced with new.","Cargo Mach.","Cargo / Ballast Systems","External Factors","","","","","Replace new washer of hatch cover cleats which was bent & bad condition.","2024-01-02T23:59:35","","Completed","2023-11-20T23:59:35","No","No","No","Internal"]
[null,null,null,32721,65254,"123_Wed Nov 15 2023 19:30:39 GMT+0800","2023-11-02T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Support Rods to be welded on the sides of the wheel jack for all covers, where the rod already exist, same has to be removed & rewelded to correct gap. ","Cargo Mach.","Cargo / Ballast Systems","External Factors","","","","","Inserting of support rods on the sides of all hatch cover wheel lifting hydraulic jack.","2024-02-02T23:59:35","","Completed","2023-12-30T23:59:35","No","No","No","Internal"]
[null,null,null,32722,30782,"123_Wed Nov 15 2023 20:38:56 GMT+0800","2023-11-02T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Rescue boat embarkation ladder safety hook on deck is thinned down, same to be replaced with shore fabricated rings.","LSA / FFA","Safety / LSA / FFA","External Factors","","","","","Replace new safety hook & rings of rescue boat embarkation ladder.","2024-01-31T23:59:35","","Completed","2024-01-30T23:59:35","No","No","No","Internal"]
[null,null,null,32724,45546,"123_Wed Nov 15 2023 19:24:52 GMT+0800","2023-11-02T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","All hatch cover hydraulic control blocks drip tray to be fabricated.","Deck - Pipe / Fittings","Cargo / Ballast Systems","External Factors","","","","","Fabricating & installing of all hatch cover hydraulic control box save-all tray.","2024-01-02T23:59:35","","Completed","2023-12-12T23:59:35","No","No","No","Internal"]
[null,null,null,32725,33736,"123_Wed Nov 15 2023 20:44:08 GMT+0800","2023-11-02T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","All 5-cargo hatch cover Hyd. motor to be oil seal to be replaced with new spares. No.1 & 3 already carried out.","Cargo Mach.","Cargo / Ballast Systems","External Factors","","","","","All cargo hatch cover hydraulic motor oil seal renewed. Presently no leakages observed.","2024-02-02T23:59:35","","Completed","2024-01-19T23:59:35","No","No","No","Internal"]
[null,null,null,32726,25389,"123_Wed Nov 15 2023 20:46:14 GMT+0800","2023-11-02T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Denso tape on all Hatch cover Hyd. motors flexible to remove & check condition, replace the hose where condition is not good.","Cargo Mach.","Cargo / Ballast Systems","External Factors","","","","","Check condition & replace new denso tape of hatch cover hydraulic motor flexible hose.","2024-02-17T23:59:35","","Completed","2024-01-27T23:59:35","No","No","No","Internal"]
[null,null,null,32727,16280,"123_Wed Nov 15 2023 20:51:10 GMT+0800","2023-11-02T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Fwd. hyd pipe till 1 Hatch cover aft needs to be blasted & painted.","Deck - Pipe / Fittings","Cargo / Ballast Systems","External Factors","","","","","Derusting & painting of No.1 cargo hold forward hydraulic pipe line .","2023-12-02T23:59:35","","Completed","2023-11-16T23:59:35","No","No","No","Internal"]
[null,null,null,32728,64773,"123_Wed Nov 15 2023 20:58:49 GMT+0800","2023-11-02T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Some Ballast Air vent inside body is rusted, same to be power tooled & painted.","Deck - Pipe / Fittings","Cargo / Ballast Systems","External Factors","","","","","Derusting & inspecting of ballast air vent on maindeck.","2023-12-31T23:59:35","","Completed","2023-12-23T23:59:35","No","No","No","Internal"]
[null,null,null,32729,66904,"123_Wed Nov 15 2023 21:00:32 GMT+0800","2023-11-02T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Fwd & Aft mast de rusting & painting to be carried out.","Navigation - Others","Navigation","External Factors","","","","","Derusting & painting of forward & aft mast.","2023-12-17T23:59:35","","Completed","2023-11-28T23:59:35","No","No","No","Internal"]
[null,null,null,32730,91554,"123_Wed Nov 15 2023 21:02:56 GMT+0800","2023-11-02T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Emg. Gen room mushroom vent mesh to be opened, derusting , painted. Edges of the vent where thinned down to be repaired.","Accommodation","Safety / LSA / FFA","External Factors","","","","","Derusting & painting of emg. generator room mushroom vent mesh.","2024-01-31T23:59:35","","Completed","2023-12-16T23:59:35","No","No","No","Internal"]
[null,null,null,32731,72503,"123_Wed Nov 15 2023 19:34:27 GMT+0800","2023-11-02T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","3 in no. of Lips of the cargo hold Booby hatch cover to welded with SS electrode","Cargo Mach.","Cargo / Ballast Systems","External Factors","","","","","Welding of cargo hold bobby hatch lips with SS electrode.","2024-01-02T23:59:35","","Completed","2023-12-26T23:59:35","No","No","No","Internal"]
[null,null,null,32732,60070,"123_Wed Nov 15 2023 20:34:41 GMT+0800","2023-11-02T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Accommodation sides & Aft side vent heads to be opened for inspection.","Accommodation","Safety / LSA / FFA","External Factors","","","","","Inspection have to carry out of accommodation sides & aft side vent heads.","2023-12-02T23:59:35","","Completed","2023-11-22T23:59:35","No","No","No","Internal"]
[null,null,null,32733,92950,"123_Wed Nov 15 2023 21:04:27 GMT+0800","2023-11-02T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Paint the aft area deck including muster stations marking.","Accommodation","Safety / LSA / FFA","External Factors","","","","","Remarking of muster station.","2023-12-02T23:59:35","","Completed","2023-11-16T23:59:35","No","No","No","Internal"]
[null,null,null,32734,97369,"123_Wed Nov 15 2023 21:08:41 GMT+0800","2023-11-02T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","All the winches brake rendering test to be carried out using new supplied kit.","Deck - Mooring Machinery","Mooring","External Factors","","","","","All mooring winches have carry out brake rendering test.","2024-01-02T23:59:35","","Completed","2023-12-18T23:59:35","No","No","No","Internal"]
[null,null,null,32735,46501,"123_Wed Nov 15 2023 21:14:38 GMT+0800","2023-11-02T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Port side gangway tends to tilt slightly on outer position after a particular location when lowering, root cause to be investigated & rectified, Same to be checked for Stbd side as well.","Deck - Machinery","Safety / LSA / FFA","External Factors","","","","","Thoroughly inspection carried out of port side pilot combination ladder, found satisfactory in condition.","2024-02-17T23:59:35","","Completed","2024-02-02T23:59:35","No","No","No","Internal"]
[null,null,null,32737,48977,"123_Wed Nov 15 2023 21:06:41 GMT+0800","2023-11-02T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","All denso tape from Coupling of LB davit hyd hoses needs to be removed & condition to be assessed, carry out power tolling, if fitting thinned down, same to be replaced with new, All hyd hoses to be replaced with new.","LSA / FFA","Safety / LSA / FFA","External Factors","","","","","Derusting & replace new denso tape of lifeboat davit hydraulic hose coupling.","2023-12-17T23:59:35","","Completed","2023-11-13T23:59:35","No","No","No","Internal"]
[null,null,null,32738,15093,"123_Wed Nov 15 2023 15:46:09 GMT+0800","2023-11-02T23:59:35","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","No.3 DG attached pump to be hauled with new spares supplied.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","AE No. 3 both LT and HT Fresh water pumps overhauled with new mechanical seal and oil seal. Aux. engine tested, found working in order.","2023-12-02T23:59:35","","Completed","2023-11-06T23:59:35","No","No","No","Internal"]
[null,null,null,32739,29245,"0_Wed Nov 15 2023 16:02:03 GMT+0800","2023-11-02T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","All the spare bearing boxes secured properly on the side plating of bottom platform & permanent securing arrangement to be fabricated with wire lashing.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","External Factors","","","","","All the spare bearing boxes on the side plating of bottom platform are secured by making permanent lashing arrangement.","2023-12-02T23:59:35","","Completed","2023-11-11T23:59:35","No","No","No","Internal"]
[null,null,null,32740,49167,"0_Wed Nov 15 2023 16:05:03 GMT+0800","2023-11-02T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ME Air cooler scavenge drain line has pin hole, same to be fabricated with new. ","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Scavenge drain line removed from place, a new section fabricated and welded in workshop and then fitted back in place. ","2024-01-02T23:59:35","","Completed","2023-11-11T23:59:35","No","No","No","Internal"]
[null,null,null,32741,28196,"0_Wed Nov 15 2023 16:07:36 GMT+0800","2023-11-02T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Sea water pipe to jacket cooler from Main line has telltale signs of leakages, same to be replaced with new.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","External Factors","","","","","A new sea water pipe section fabricated and fitted back in place.","2023-12-17T23:59:35","","Completed","2023-11-10T23:59:35","No","No","No","Internal"]
[null,null,null,32742,95253,"0_Wed Nov 15 2023 15:59:12 GMT+0800","2023-11-02T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","some lagging in ER to be replaced, material onboard. a) TC piping, boiler blow down v/v & pipe c) steam drain line behind TC platform.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","External Factors","","","","","Following laggings in ER replaced:\na) TC piping, boiler blow down v/v & pipe c) steam drain line behind TC platform.","2024-01-02T23:59:35","","Completed","2023-11-10T23:59:35","No","No","No","Internal"]
[null,null,null,32743,76896,"0_Wed Nov 15 2023 16:19:56 GMT+0800","2023-11-02T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","To fabricate the backwash arrangement for LO cooler SW side.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Main engine LO cooler back flushing arrangement fabricated and fitted in place","2023-12-17T23:59:35","","Completed","2023-11-09T23:59:35","No","No","No","Internal"]
[null,null,null,32744,80364,"0_Wed Nov 15 2023 16:21:51 GMT+0800","2023-11-02T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","FO transfer pp mech seal slightly leaking, same to be replace with new spare.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","","","","","FO transfer pump, old gland packings removed and new gland packings fitted, now no leakages observed.","2023-12-17T23:59:35","","Completed","2023-11-11T23:59:35","No","No","No","Internal"]
[null,null,null,32745,32947,"0_Wed Nov 15 2023 16:17:26 GMT+0800","2023-11-02T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","OWS sample vv to be sealed from unions & update the same in sealing list. Maker 5 yearly calibration certificate to be posted near to OWS. Direct Bilge suct. v/v to be also sealed.","Documentation","Eng. / Strg. Comp.","External Factors","","","","","OWS sample valve sealed from unions and seal record updated. Maker 5 yearly calibration certificate posted near OWS. Direct Bilge suction valve sealed.","2023-11-17T23:59:35","","Completed","2023-11-11T23:59:35","No","No","No","Internal"]
[null,null,null,32746,24109,"0_Wed Nov 15 2023 16:09:54 GMT+0800","2023-11-02T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Main Engine FO Auto backwash filter shaft seal leaking slightly, same to be replaced with new one.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Main engine FO Autobackwash filter shaft dismantled and seal renewed. Now no leakages observed.","2023-12-02T23:59:35","","Completed","2023-11-08T23:59:35","No","No","No","Internal"]
[null,null,null,32747,59318,"0_Wed Nov 15 2023 16:23:59 GMT+0800","2023-11-02T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Main Cooling SW pps have slight leakage from seals, same to be clean & refitted, then check for leakages.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","","","","","Both Main cooling sea water pump, mechanical seal cover bolt removed, cleaned stator and rotor part of mechanical seal with fresh water, currently no leakages observed.","2023-12-02T23:59:35","","Completed","2023-11-11T23:59:35","No","No","No","Internal"]
[null,null,null,32748,44853,"0_Wed Nov 15 2023 15:56:12 GMT+0800","2023-11-02T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","LO Auto backwash filter spare candles to clean using maker cleaning kit & procedure & secure properly.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","LO Auto backwash filter spare candles cleaned using maker cleaning kit and procedure and rapped each candle after cleaning with plastic and safely secured.","2023-12-02T23:59:35","","Completed","2023-11-13T23:59:35","No","No","No","Internal"]
[null,null,null,32749,49402,"123_Wed Nov 15 2023 19:38:44 GMT+0800","2023-11-02T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Safety walkway on port side to be rigged & additional chain where required to be added with D-shackles.","Miscellaneous","Safety / LSA / FFA","External Factors","","","","","Rigging of safety line on port side main deck walkway.","2023-12-02T23:59:35","","Completed","2023-11-07T23:59:35","No","No","No","Internal"]
[null,null,null,32750,38808,"123_Wed Nov 15 2023 19:44:26 GMT+0800","2023-11-02T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Shower fittings 4 in number supplied to be fitted in leaking bathrooms. 2 new supplied tap to be fitted in galley & 2 new flexible hoses to be fitted in galley.","Accommodation","MLC Related","External Factors","","","","","Replace new shower fitting & tap which was bad condition & leakage.","2023-11-17T23:59:35","","Completed","2023-11-03T23:59:35","No","No","No","Internal"]
[null,null,null,32751,97844,"123_Wed Nov 15 2023 19:49:38 GMT+0800","2023-11-02T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","All cabin portholes to check for leakage & repairs de rusting to be carried out on the bulkhead where water is leaking after arresting the leaks. All defects identified during cabin rounds to be rectified.","Accommodation","MLC Related","External Factors","","","","","Derusting & painting of crew's cabin portholes which was bad condition & leaked.","2023-12-17T23:59:35","","Completed","2023-11-14T23:59:35","No","No","No","Internal"]
[null,null,null,32752,30695,"123_Wed Nov 15 2023 20:00:37 GMT+0800","2023-11-02T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","LB lowering to be carried out & secure properly in its place.","LSA / FFA","Safety / LSA / FFA","Knowledge Based","","","","","Carry out lowering, launching & manoeuvring  of life boat .","2023-11-17T23:59:35","","Completed","2023-11-09T23:59:35","No","No","No","Internal"]
[null,null,null,32753,83358,"123_Wed Nov 15 2023 20:49:20 GMT+0800","2023-11-02T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","All greasing points on deck to make a list & color code yellow, greasing of windlass & winches gear to be carried out with special grease.","Deck - Mooring Machinery","Mooring","External Factors","","","","","Replace new grease nipple which was missing & bad condition of winches & windlass and mark with yellow.","2024-01-02T23:59:35","","Completed","2023-11-13T23:59:35","No","No","No","Internal"]
[null,null,null,32754,74900,"123_Wed Nov 15 2023 20:54:40 GMT+0800","2023-11-02T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","U clamps conditions to be checked & thinned down clamps to be replaced with new as marked.","Deck - Pipe / Fittings","Cargo / Ballast Systems","External Factors","","","","","Replace new U clamps on main deck hydraulic line & other pipe lines.","2024-01-02T23:59:35","","Completed","2023-11-07T23:59:35","No","No","No","Internal"]
[null,null,null,32755,66324,"123_Wed Nov 15 2023 20:57:06 GMT+0800","2023-11-02T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Forward embarkation ladder to be secured properly with D shackle. New canvas to be fitted to be fitted for Embarkation ladder.","LSA / FFA","Safety / LSA / FFA","External Factors","","","","","Replace new canvas cover & secure of forward embarkation ladder.","2023-11-17T23:59:35","","Completed","2023-11-04T23:59:35","No","No","No","Internal"]
[null,null,null,32756,32926,"123_Wed Nov 15 2023 21:10:39 GMT+0800","2023-11-02T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Ships office and officer smoke room curtain needs to be hard washed as there are stain marks on them","Accommodation","Crew Management","External Factors","","","","","Hard washing of ship's office & officer smoke room curtain.","2023-12-02T23:59:35","","Completed","2023-11-12T23:59:35","No","No","No","Internal"]
[null,null,null,32757,25313,"123_Wed Nov 15 2023 20:36:43 GMT+0800","2023-11-02T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","BNWAS box to be secured properly on bridge. ","Navigation - VDR / BNWAS","Navigation","External Factors","","","","","Secured of BNWAS panel box on bridge.","2023-12-02T23:59:35","","Completed","2023-11-14T23:59:35","No","No","No","Internal"]
[null,null,null,32758,20200,"0_Wed Nov 15 2023 16:30:28 GMT+0800","2023-11-02T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Galley aircon Condenser Cooling Sea water inlet pipe has telltale sign of leakage, same to be fabricated with new.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","The sea water outlet pipe section fabricated and fitted. Presently no leakages observed.","2023-12-02T23:59:35","","Completed","2023-11-17T23:59:35","No","No","No","Internal"]
[null,null,null,32759,35504,"0_Wed Nov 15 2023 15:52:03 GMT+0800","2023-11-02T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Both the sea chest internal mesh to be fitted to obstruct the passage of muck passing through the holes & checking the coolers.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","The holes of mesh are very small. The problem identified as the strainer opening was not exactly matching with sea water inlet at strainer therby bypassing the sea growth. Locking arrangement of stainless steel fabricated and welded to strainer in such a way that the strainer opening and sea water inlet is matching and nobypassing of sea growth and other foreigh materialas will take place.","2023-12-02T23:59:35","","Completed","2023-11-21T23:59:35","No","No","No","Internal"]
[null,null,null,32760,79931,"123_Wed Nov 15 2023 21:12:36 GMT+0800","2023-11-02T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","4 Chairs seats in Ships office to be fabricated with spare cloth.","Accommodation","MLC Related","External Factors","","","","","Replace new chairs in ship's office which was received in singapore.","2023-11-17T23:59:35","","Completed","2023-11-03T23:59:35","No","No","No","Internal"]
[null,null,null,33267,18491,"0_Wed Nov 29 2023 18:51:40 GMT+0800","2023-11-18T23:59:35","Observation","Ship Staff","Ship Staff Insp.","AE port side jacket water cooler No. 2- found sea water outlet line leaking.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","External Factors","","","","","A new sea water outlet line fabricated and fitted in place. No further leakages observed.","2023-12-31T23:59:35","","Completed","2023-11-20T23:59:35","No","No","No","Internal"]
[null,null,null,33269,37057,"123_Wed Nov 29 2023 19:03:52 GMT+0800","2023-11-20T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Incinerator waste oil Service tank: It was observed that the oil/sludge in both waste oil service tank is not getting hot. Water also not evaporating from waste oil service tank.","Hull & Tanks","Eng. / Strg. Comp.","External Factors","","","","","The heating coil return line steam trap inspected and cleaned.  One by one both tanks were emptied, cleaned and observed a thick salt deposits on heating coil. The same cleaned. Now very good evaporation rate is observed.","2023-12-31T23:59:35","","Completed","2023-11-27T23:59:35","No","No","No","Internal"]
[null,null,null,32736,84493,"123_Wed Nov 22 2023 14:48:14 GMT+0800","2023-11-21T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp."," LOCTITE 5910 to apply on all the stay bolts (Between Stay bolt nut & mating surface A-Frame) as well as cylinder head bolts which enters into A-frame. ","E/R - Main Engine","Eng. / Strg. Comp.","External Factors,Equipment Related","","","","","All ME stay bolts  (Between Stay bolt nut & mating surface A-Frame) as well as cylinder head bolts which enters into A-frame  applied with loctite 5910 to prevent water ingress through these into sump after receiving LOCTITE 5910.","2024-01-30T23:59:35","PELA230346","Completed","2024-01-05T23:59:35","No","No","No","Internal"]
[null,null,null,33272,36071,"123_Wed Nov 29 2023 18:45:06 GMT+0800","2023-11-21T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Boiler feed water pump No. 1 observed to be leaking from mechanical seal.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","","","","","The feed water pump No. 1 overhauled. All parts thoroughly cleaned and inspected. All clearances found within limits as per makers guidelines. The mechanical seal renewed. ","2023-12-31T23:59:35","","Completed",null,"No","No","No","Internal"]
[null,null,null,33266,27693,"123_Wed Nov 29 2023 18:48:14 GMT+0800","2023-11-22T23:59:35","Observation","Ship Staff","Ship Staff Insp.","ME Fuel oil circulating pump No. 1 leaking from gland packing.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","","","","","ME fuel oil circulating pump gland packing renewed. Presently no leakages observed.","2023-12-31T23:59:35","","Completed","2023-11-27T23:59:35","No","No","No","Internal"]
[null,null,null,33268,58999,"123_Wed Nov 29 2023 18:54:45 GMT+0800","2023-11-25T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Low sea chest- observed sea water leaking from one of the anode flange.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","External Factors","","","","","The sea chest strainer cover removed and anode packing renewed. The cover fitted in place, the sea chest is in use with no further leakages observed.","2023-12-31T23:59:35","","Completed","2023-11-28T23:59:35","No","No","No","Internal"]
[null,null,null,33273,70963,"123_Fri Dec 15 2023 14:58:40 GMT+0800","2023-12-02T23:59:35","Observation","Ship Staff","Ship Staff Insp.","To Fabricate new pipe section for AE jacket cooler inlet line from Main Cooling Sea water pump as it found leaking as the pipe line observed to have hole.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","External Factors","","","","","The pipe section removed from place, brought to workshop, found completely wasted due to corrosion. A new section fabricated and fitted in place. The system tested, no further leakages observed. The pipeline coated with primer and then painted.","2023-12-31T23:59:35","","Completed","2023-12-04T23:59:35","No","No","No","Internal"]
[null,null,null,33270,76339,"123_Fri Dec 15 2023 15:01:36 GMT+0800","2023-12-04T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Fresh water hydrophore pump not taking suction from center tank. To investigate and troubleshoot.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","External Factors","","","","","W HYDROPHORE PUMP SUCTION PIPE FROM FW CENTRE TANK TAKEN OUT,AS FOUND THE PUMP WAS NOT TAKING SUCTION FROM THE CENTRE TANK. DURING INSPECTION,FOUND BLOCKED INSIDE THE PIPE WITH RAGS WHICH WAS LEFT DURING CLEANING TANK IN PAST AND RUBBER COATING INSIDE THE PIPE DAMAGED. SAME PIPE SECTION NEWLY FABRICATED AND FITTED BACK IN PLACE.","2023-12-31T23:59:35","","Completed","2023-12-07T23:59:35","No","No","No","Internal"]
[null,null,null,33271,19737,"0_Fri Dec 15 2023 15:04:11 GMT+0800","2023-12-08T23:59:35","Observation","Ship Staff","Ship Staff Insp.","TO FABRICATE AND REPLACE FIRE LINE PIPE SECTION NEAR AIR RESERVOIR ON 3RD DECK PLATFORM DUE TO LEAKAGE AND CORROSION","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","External Factors","","","","","ENGINE ROOM FIRE LINE PIPE SECTION FOUND LEAKY AND CORRODED , SAME REMOVED AND BROUGHT TO WORKSHOP,NEWLY FABRICATED THE SAME. APPLIED TWO COAT OF EPOXY PAINT INSIDE THE PIPE AND PIPE FITTED BACK WITH NEW GASKETS. FIRE & GS PUMP TRIED OUT;CHECKED FOR LEAKAGES.ALL FOUND SATISFACTORY. ","2023-12-25T23:59:35","","Completed","2023-12-11T23:59:35","No","No","No","Internal"]
[null,null,null,33274,12736,"0_Fri Dec 15 2023 15:07:21 GMT+0800","2023-12-09T23:59:35","Observation","Ship Staff","Suptd. Insp.","PURIFIER ROOM EXHAUST BLOWER FLAPS OPERATING CYLINDER MALFUNCTIONING.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","PURIFIER ROOM EXHAUST BLOWER FLAPS OPERATING CYLINDER FOUND STUCK ,SAME TAKEN OUT TO THE WORKSHOP;OVERHAULED. DURING INSPECTION FOUND MOISTURE AND DUST DEPOSITED AROUND PISTON. ALL PARTS THOROUGHLY CLEANED AND  ALL PARTS CONDITION FOUND SATISFACTORY.SAME BOXED BACK AND FITTED BACK IN PLACE.BLOWER FLAP OPERATION TRIED OUT,FOUND WORKING SATISFACTORY.","2023-12-27T23:59:35","","Completed","2023-12-12T23:59:35","No","No","No","Internal"]
[null,null,null,33275,24305,"123_Fri Dec 15 2023 16:42:51 GMT+0800","2023-12-11T23:59:35","Observation","Ship Staff","Ship Staff Insp.","GALLEY A/C CONDENSER S.W OUTLET PIPE SECTION FOUND LEAKY AND CORRODED.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","GALLEY A/C CONDENSER SEA WARER OUTLET PIPE FOUND LEAKY AND CORRODED. SAME PIPE SECTION TAKEN OUT AND BROUGHT TO WORKSHOP. SAME NEWLY FABRICATED AND FITTED BACK WITH NEW GASKET IN PLACE. SEA WATER OPENED TO CHECK FOR LEAKAGES. FOUND NO LEAKAGE. GALLEY A/C PUT INTO SERVICE. ","2023-12-31T23:59:35","","Completed","2023-12-14T23:59:35","No","No","No","Internal"]
[null,null,null,33610,27267,"123_Mon Jan 15 2024 21:59:15 GMT+0800","2023-12-16T23:59:35","Observation","Ship Staff","Ship Staff Insp.","BWTS, DISINFECTANT PUMP SUCTION  PIPE SECTION AND DELIVERY PIPE SECTION ,FOUND CORRODED AND LEAKY.","E/R - Pipes/ valves & fittings","Cargo / Ballast Systems","Equipment Related","","","","","BWTS, DISINFECTANT PUMP SUCTION  PIPE SECTION AND DELIVERY PIPE SECTION ,FOUND CORRODED AND LEAKY. SAME REMOVED AND BROUGHT TO WORKSHOP,NEWLY FABRICATED AND FITTED BACK WITH NEW GASKET.","2024-01-30T23:59:35","","Completed","2023-12-18T23:59:35","No","No","No","Internal"]
[null,null,null,33616,16823,"123_Mon Jan 15 2024 22:06:19 GMT+0800","2023-12-17T23:59:35","Observation","Ship Staff","Ship Staff Insp.","BWTS, DISINFECTANT PUMP ,01 NO DELIVERY PIPE SECTION  FOUND CORRODED AND LEAKY.","E/R - Pipes/ valves & fittings","Cargo / Ballast Systems","Equipment Related","","","","","BWTS, DISINFECTANT PUMP ,DELIVERY PIPE SECTION ,FOUND CORRODED AND LEAKING, SAME REMOVED AND BROUGHT TO WORKSHOP, NEWLY FABRICATED AND FITTED BACK WITH THE NEW GASKET.","2024-01-31T23:59:35","","Completed","2023-12-19T23:59:35","No","No","No","Internal"]
[null,null,null,33611,41838,"123_Mon Jan 15 2024 22:14:41 GMT+0800","2023-12-20T23:59:35","Observation","Ship Staff","Ship Staff Insp."," FUEL OIL PURIFIER SLUDGE TANK SUCTION VALVE TO SLUDGE PUMP FOUND CHOKED DURING INTERNAL TRANSFER OF SLUDGE.","E/R - Pipes/ valves & fittings","General Appearance","Equipment Related","","","",""," FUEL OIL PURIFIER SLUDGE TANK SUCTION VALVE TO SLUDGE PUMP FOUND CHOKED DURIN INTERNAL TRANSFER OF SLUDGE. SAME OPENED UP AND OVERHAULED. ON INSPECTION FOUND SLUDGE DEPOSITED INSIDE VALVE. SLUDGE DEPOSITS CLEANED AND VALVE FITTED BACK WITH NEW GASKETS.","2024-01-30T23:59:35","","Completed","2023-12-21T23:59:35","No","No","No","Internal"]
[null,null,null,33617,40145,"123_Mon Jan 15 2024 22:26:27 GMT+0800","2023-12-20T23:59:35","Observation","Ship Staff","Ship Staff Insp.","BALLAST PUMP #2 SUCTION VALVE FROM BALLAST TANKS WAS FOUND VERY HARD TO OPEN AND CLOSE.","E/R - Air Comp.,E/R - Pipes/ valves & fittings","General Appearance","Equipment Related","","","","","BALLAST PUMP #2 SUCTION VALVE FROM BALLAST TANKS WAS FOUND VERY HARD TO OPEN AND CLOSE.DURING INSPECTION,FOUND  BUTTERFLY VALVE OPERATING GEAR BOX  JAMMED.SAME TAKEN OUT AND OVERHAULED ,ALL PARTS THOROUGHLY CLEANED AND GREASING CARRIED OUT AND MADE IT FREE. GEAR BOX BOXED BACK AND FITTED IN PLACE. CHECKED FOR THE OPERATION OF VALVE,ALL FOUND SATISFACTORY.","2024-01-30T23:59:35","","Completed","2023-12-22T23:59:35","No","No","No","Internal"]
[null,null,null,33612,32668,"123_Mon Jan 15 2024 22:40:05 GMT+0800","2023-12-23T23:59:35","Defect","Ship Staff","Ship Staff Insp.","EXISTING AUX. BOILER ATMOSPHERIC CONDENSER 12 NOS TUBES PLUGED IN DUE TO LEAK WHICH DECREASE THE CONDENSER EFFICIENCY. VESSEL PLANNED TO RPLACE WITH NEW CONDENSER UPON RECEIVING THE NEW SPARE.","E/R - Boiler","General Appearance","Equipment Related","","","",""," EXISTING ATMOSPHERIC CONDENSOR REPLACED WITH NEWLY RECEIVED ATMOSPHERIC CONDENSOR.ALL CONNECTIONS DISMOUNTED FROM THE EXISTING ATMOSPHERIC CONDENSOR.CONDENSOR TAKEN OUT FROM THE BASE AND NEW CONDENSOR SHIFTED TO THE SAME BASE.ALL CONNECTIONS REMOUNTED WITH THE NEW GASKET.CONDENSOR'S SEA WATER INLET AND OUTLET TEMPERATURE GUAGES RENEWED.CONDENSOR'S ANODE INSPECTED,FOUND IN GOOD ORDER.SEA WATER AND STEAM OPENED FOR THE CONDENSOR.CHECKED FOR LEAKAGES AND ANY ABNORMALITIES.ALL FOUND SATISFACTORY.","2024-01-31T23:59:35","","Completed","2023-12-29T23:59:35","No","No","No","Internal"]
[null,null,null,33620,50307,"123_Tue Jan 16 2024 03:07:27 GMT+0800","2023-12-30T23:59:35","Observation","Others (Eg. Insurance etc.)","Others (Eg. Insurance etc.)","MAGNETIC COMPASS AIR BUBBLE 2CM\n\n","Navigation - Others","Navigation","Human Error","","","","","The air bubble removed immediately and supporting liquid filled ","2024-01-02T23:59:35","","Completed","2023-12-30T23:59:35","No","No","No","External"]
[null,null,null,33621,94786,"123_Tue Jan 16 2024 03:00:54 GMT+0800","2023-12-30T23:59:35","Observation","Others (Eg. Insurance etc.)","Others (Eg. Insurance etc.)","Two Fire doors to steering gear rooms and deck-C locks damaged. Two fire doors upper deck stairway and to provision room in galley packing partly missing","Accommodation,Miscellaneous","Eng. / Strg. Comp.","External Factors","","","","","The steering gear door lock arrangement renewed and tested, found operating satisfactorily.\nThe C deck door lock assembly removed, cleaned, lubricated and fitted back. Now the door locking arrangement is operating smoothly.\nThe Vessel placed the missing fire- retardant packing at the bottom of the door frame of both these doors before PSC inspector disembarked.\nThese rectifications were reported to PSC and defects were closed.\n","2024-01-02T23:59:35","","Completed","2023-12-30T23:59:35","No","No","No","External"]
[null,null,null,33622,28736,"123_Tue Jan 16 2024 03:03:46 GMT+0800","2023-12-30T23:59:35","Observation","Others (Eg. Insurance etc.)","Others (Eg. Insurance etc.)","Certificate for full body protective suit not submitted during inspection","Documentation","Cert. & Docu.","Human Error","","","","","The soft copy of the type approval certificate was downloaded from the maker’s website and provided for closure. Fixed and reported to PSCI and Defect closed. ","2024-01-02T23:59:35","","Completed","2023-12-30T23:59:35","No","No","No","External"]
[null,null,null,33613,88138,"123_Mon Jan 15 2024 22:58:34 GMT+0800","2024-01-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","01 NO DEFECTIVE PILOT LADDER AIR MOTOR RECEIVED FROM THE DECK AS IT FOUND NOT WORKING PROPERLY AT THE TIME OF LIFTING PILOT LADDER. ","Deck - Machinery","General Appearance","Equipment Related","","","","","01 NOS. DEFECTIVE PILOT LADDER AIR MOTOR RECEIVED FROM THE DECK AS IT FOUND NOT WORKING PROPERLY AT THE TIME OF LIFTING PILOT LADDER. SAME TAKEN OUT AND BROUGHT TO WORKSHOP FOR OVERHAULING. ON INSEPECTION IT WAS FOUND THAT THE OPERATING HANDLE WAS STUCK AND ROTOR BLADE WEAR DOWN AND BROKEN. ROTOR BLADE REPLACED WITH NEW SPARE. OPERATING HANDLE FOUND RUSTED, SAME CLEANED AND GREASING CARRIED OUT. HANDLE FITED BACK AND AIR MOTOR BOXED BACK. AIR MOTOR FITTED IN PLACE AND PILOT LADDER OPERATION TRIED OUT. FOUND WORKING SATISFACTORILY.","2024-01-30T23:59:35","","Completed","2024-01-04T23:59:35","No","No","No","Internal"]
[null,null,null,33614,20420,"123_Mon Jan 15 2024 23:14:31 GMT+0800","2024-01-06T23:59:35","Observation","Ship Staff","Ship Staff Insp.","DURING INSPECTION NO.1 E/R VENT FAN DAMPER AND PURIFIER EXHAUST FAN DAMPER ACTUATOR CYLINDER FOUND LEKAY AND NOT WORKING PROPERLY.","E/R - Aux. Mach.","Emgcy. Systems","Equipment Related","","","","","DURING INSPECTION OF  NO.1 E/R AIR VENT FAN AND PURIFIER EXHAUST FAN DAMPER FOUND THAT AIR CYLINDER FOR CLOSING  VENT DAMPER WAS NOT CLOSING POPERLEY AND AIR IS LEAKING ON UPPER PART OF CYL.  CYLINDER REPLACED WITH NEW RECEIVED SPARE TRIED OUT FOUND CLOSING SATISFACTORY BUT WHEN AIR IS  RELEASED SPRING CANNOT OPEN THE DAMPER. PUT BACK OLD  SPRING AND TRIED OUT ALL WORKING SATISFACTORY. ","2024-01-30T23:59:35","","Completed","2024-01-08T23:59:35","No","No","No","Internal"]
[null,null,null,33615,85383,"123_Mon Jan 15 2024 23:16:59 GMT+0800","2024-01-06T23:59:35","Observation","Ship Staff","Ship Staff Insp.","BWTS, DISINFECTANT PUMP DELIVERY SIDE 01 NOS. BRANCH PIPE FOUND CORRODED AND LEAKY","E/R - Pipes/ valves & fittings","General Appearance","Equipment Related","","","","","BWTS, DISINFECTANT PUMP DELIVERY SIDE 01 NOS. BRANCH PIPE FOUND CORRODED AND LEAKY.SAME TAKEN OUT TO THE WORKSHOP,NEWLY FABRICATED AND FITTED IN PLACE WITH NEW GASKETS.APPLIED PRIMER COATING ON THE PIPE.","2024-01-31T23:59:35","","Completed","2024-01-08T23:59:35","No","No","No","Internal"]
[null,null,null,33618,42065,"123_Mon Jan 15 2024 23:20:49 GMT+0800","2024-01-07T23:59:35","Observation","Ship Staff","Ship Staff Insp.","MAIN ENGINE FUEL OIL AUTOBACK WASH FILTER AND AUX ENGINE AUTO BACKWASH FILTER WAS FOUND NOT WORKING PROPERLY.","E/R - Pipes/ valves & fittings","General Appearance","Equipment Related","","","","","MAIN ENGINE FUEL OIL AUTOBACK WASH FILTER AND AUX ENGINE AUTO BACKWASH FILTER WAS FOUND NOT WORKING PROPERLY.SAME REMOVED AND OVERHAULED.ON INSPECTION IT WAS FOUND THAT THE FILTER'S AIR DRIVING UNIT PISTON O RINGS WAS DAMAGED,SAME RENEWED AND FILTER BOXED BACK. FILTER TRIED OUT , ALL FOUND WORKING SATISFACTORY.","2024-01-30T23:59:35","","Completed","2024-01-09T23:59:35","No","No","No","Internal"]
[null,null,null,33619,34629,"123_Mon Jan 15 2024 23:22:50 GMT+0800","2024-01-08T23:59:35","Observation","Ship Staff","Ship Staff Insp.","AE JACKET COOLER SEA WATER OUTLET PIPE SECTION FOUND LEAKY AND CORRODED.","E/R - Pipes/ valves & fittings","General Appearance","Equipment Related","","","",""," AE JACKET COOLER SEA WATER OUTLET PIPE SECTION FOUND LEAKY AND CORRODED.SAME TAKE OUT TO THE WORKSHOP AND FABRICATED.EPOXY PAINTING CARRIED OUT ON THE PIPE SECTION.SAME FITTED BACK WITH NEW GASKETS.COOLER TRIED OUT ,FOUND NO SIGN OF LEAKAGES.ALL FOUND IN GOOD ORDER.","2024-01-31T23:59:35","","Completed","2024-01-09T23:59:35","No","No","No","Internal"]
[null,null,null,34361,99318,"123_Thu Feb 15 2024 20:01:06 GMT+0800","2024-01-13T23:59:35","Defect","Ship Staff","Ship Staff Insp.","BWTS TRO UNIT NO. 2, Main PCB is faulty.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","Received TRO Unit PCB at Singapore on 3rd February 2024.  PCB renewed and the system is working satisfactorily.","2024-02-29T23:59:35","PELA240016","Completed","2024-02-03T23:59:35","No","No","No","Internal"]
[null,null,null,33897,23648,"0_Wed Jan 31 2024 19:00:22 GMT+0800","2024-01-15T23:59:35","Observation","Ship Staff","Ship Staff Insp."," CLAMPING ARRANGEMENTS FOR SECURING THE MAIN ENGINE SPARE PISTON FOUND MISSING.","Miscellaneous","Eng. / Strg. Comp.","External Factors","","","",""," CLAMPING ARRANGEMENTS FABRICATED FOR SECURING THE MAIN ENGINE SPARE PISTON AND FITTED IN PLACE.","2024-02-10T23:59:35","","Completed","2024-01-16T23:59:35","No","No","No","Internal"]
[null,null,null,33896,15540,"0_Wed Jan 31 2024 18:57:39 GMT+0800","2024-01-16T23:59:35","Observation","Ship Staff","Ship Staff Insp.","DURING ROUTINE INSPECTION ON ENGINE ROOM, SOME OF THE ENGINE ROOM PUMP'S COUPLING SAFETY GUARD WERE FOUND MISSING","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","","","",""," DURING ROUTINE INSPECTION ON ENGINE ROOM, SOME OF THE ENGINE ROOM PUMP'S COUPLING SAFETY GUARD WERE FOUND MISSING.NEW GUARD FABRICATED AND FITTED IN PLACE.\nLOCATION: 1) PORT USE SW PUMP.\n                    2) FWG EJECTOR PUMP.\n                    3) FO TRANSFER PUMP.","2024-02-10T23:59:35","","Completed","2024-01-19T23:59:35","No","No","No","Internal"]
[null,null,null,33893,95480,"0_Wed Jan 31 2024 18:55:08 GMT+0800","2024-01-18T23:59:35","Observation","Ship Staff","Ship Staff Insp.","AE#1 FUEL OIL LINE QUICK CLOSING VALVE WAS NOT OPERATING PROPERLY","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","AE#1 FUEL OIL LINE QUICK CLOSING VALVE WAS NOT OPERATING PROPERLY.SAME OPENED UP, FOUND O RINGS OF AIR PISTON WAS DAMAGED,SAME RENEWED AND BOXED BACK. QCV TRIED OUT,FOUND WORKING SATISFACTORY.","2024-02-10T23:59:35","","Completed","2024-01-20T23:59:35","No","No","No","Internal"]
[null,null,null,33898,78749,"0_Wed Jan 31 2024 18:53:06 GMT+0800","2024-01-18T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Three light fixtures outside accommodation found damaged.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","External Factors","","","","","THREE LIGHT FIXTURES CHANGED OUTSIDE ACCOMODATION AT D & B DECK-WORKING SATISFACTORY.","2024-02-10T23:59:35","","Completed","2024-01-24T23:59:35","No","No","No","Internal"]
[null,null,null,33894,14442,"0_Wed Jan 31 2024 18:46:44 GMT+0800","2024-01-22T23:59:35","Observation","Ship Staff","Ship Staff Insp.","ENGINE ROOM , THIRD DECK LEVEL ;STBD SIDE FIRE HYDRANT 01NOS. FOUND LEAKING.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","ENGINE ROOM , THIRD DECK LEVEL ;STBD SIDE FIRE HYDRANT 01NOS. FOUND LEAKING.SAME REPLACED WITH NEW SPARE VALVE WITH NEW GASKETS.FIRE PUMP TRIED OUT.NO SIGN OF LEAKS OBSERVED.","2024-02-10T23:59:35","","Completed","2024-01-26T23:59:35","No","No","No","Internal"]
[null,null,null,33895,93261,"0_Wed Jan 31 2024 18:44:12 GMT+0800","2024-01-27T23:59:35","Observation","Ship Staff","Ship Staff Insp.","FIRE BILGE &GS PUMP #1 DISCHARGE SIDE PIPE SECTION TO THE MAIN FIRE LINE WAS FOUND LEAKING.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","FIRE BILGE &GS PUMP #1 DISCHARGE SIDE PIPE SECTION TO THE MAIN FIRE LINE WAS FOUND LEAKING.SAME BROUGHT TO WORKSHOP,FABRICATED AND FITTED BACK WITH NEW GASKETS.FIRE PUMP TRIED OUT, NO SIGN OF LEAKS OBSERVED.","2024-02-10T23:59:35","","Completed","2024-01-29T23:59:35","No","No","No","Internal"]
[null,null,null,33892,87145,"123_Wed Jan 31 2024 18:41:50 GMT+0800","2024-01-29T23:59:35","Observation","Ship Staff","Ship Staff Insp."," AUXILARY ENGINE JACKET FRESH WATER COOLER #2 SEA WATER PIPE SECTION FOUND LEAKING.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","",""," AUXILARY ENGINE JACKET FRESH WATER COOLER #2 SEA WATER PIPE SECTION FOUND LEAKING.SAME REMOVED ,BROUGHT TO WORKSHOP;FABRICATED AND FITTED BACK WITH NEW GASKETS.COOLER TRIED OUT.NO SIGN OF LEAKS OBSERVED.","2024-02-10T23:59:35","","Completed","2024-01-30T23:59:35","No","No","No","Internal"]
[null,null,null,34354,64946,"123_Thu Feb 15 2024 09:43:20 GMT+0800","2024-02-03T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Paint locker to be arranged properly","Miscellaneous","General Appearance","External Factors","","","","","","2024-03-31T23:59:35","","Completed","2024-03-02T23:59:35","No","No","No","Internal"]
[null,null,null,34356,59722,"0_Thu Feb 15 2024 09:48:38 GMT+0800","2024-02-03T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Few drain plugs of the save alls on deck to be lashed with wire or chain","Miscellaneous","MARPOL Related","External Factors","","","","","","2024-03-31T23:59:35","","Completed","2024-03-02T23:59:35","No","No","No","Internal"]
[null,null,null,34357,91711,"0_Wed Feb 14 2024 21:26:00 GMT+0800","2024-02-03T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ME flywheel pit to be cleaned.","Miscellaneous","Eng. / Strg. Comp.","External Factors","","","","","ME Flywheel pit cleaned.","2024-02-18T23:59:35","","Completed","2024-02-14T23:59:35","No","No","No","Internal"]
[null,null,null,34358,71772,"0_Tue Feb 13 2024 16:50:29 GMT+0800","2024-02-03T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ME jacket cooling FW inlet /outlet pipes near fwd aux blower, to be covered with insulation lagging.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","External Factors","","","","","ME jacket cooling FW inlet /outlet pipes near fwd aux blower, covered with insulation lagging.","2024-03-04T23:59:35","","Completed","2024-02-12T23:59:35","No","No","No","Internal"]
[null,null,null,34359,31449,"0_Thu Feb 15 2024 09:46:36 GMT+0800","2024-02-03T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","All wire ropes in fore peak store to be identified and marked","Miscellaneous","General Appearance","External Factors","","","","","Inventory of spare wire ropes in bosun store carried out & record maintained properly.","2024-02-18T23:59:35","","Completed","2024-02-12T23:59:35","No","No","No","Internal"]
[null,null,null,34360,37278,"123_Wed Feb 14 2024 21:04:28 GMT+0800","2024-02-03T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Bridge wing fire hydrant pressure gauge root valve to be renewed","Deck - Pipe / Fittings","Safety / LSA / FFA","External Factors","","","","","Bridge wing fire hydrant root valve and pressure gauge renewed.","2024-02-12T23:59:35","","Completed","2024-02-12T23:59:35","No","No","No","Internal"]
[null,null,null,34362,66995,"0_Wed Feb 14 2024 21:15:10 GMT+0800","2024-02-03T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Main engine FO high pressure pipes to be arrange properly .Defective ones to be overhauled or discarded.","Miscellaneous","Eng. / Strg. Comp.","External Factors","","","","","Main engine high pressure pipes properly secured on top of ECR deck by fabricating clamping arrangement. Old defective high pressure pipes discarded.","2024-02-18T23:59:35","","Completed","2024-02-15T23:59:35","No","No","No","Internal"]
[null,null,null,34367,80377,"0_Wed Feb 14 2024 21:21:02 GMT+0800","2024-02-03T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","FWG sight glass to be cleaned","Miscellaneous","Eng. / Strg. Comp.","External Factors","","","","","FWG sight glass cleaned.","2024-02-18T23:59:35","","Completed","2024-02-13T23:59:35","No","No","No","Internal"]
[null,null,null,34368,72774,"123_Wed Feb 14 2024 21:19:45 GMT+0800","2024-02-03T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","AE CFW cooler- Defective & missing thermometers to be replaced.","Miscellaneous","Eng. / Strg. Comp.","External Factors","","","","","AE CFW cooler- Defective & missing thermometers renewed.","2024-02-18T23:59:35","","Completed","2024-02-12T23:59:35","No","No","No","Internal"]
[null,null,null,34369,86755,"0_Wed Feb 14 2024 21:09:43 GMT+0800","2024-02-03T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","AC compressor body cosmetic condition is not good. To remove the old paint & repaint.","Accommodation","General Appearance","External Factors","","","","","AC compressor body and condenser old paint removed and re applied with fresh paint. The dip tray also cleaned and p[ainted.","2024-03-04T23:59:35","","Completed","2024-02-13T23:59:35","No","No","No","Internal"]
[null,null,null,34370,81056,"123_Tue Feb 13 2024 16:46:53 GMT+0800","2024-02-03T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Main engine flywheel pit to be cleaned.\n","Miscellaneous","Eng. / Strg. Comp.","External Factors","","","","","Main engine flywheel pit cleaned.","2024-02-20T23:59:35","","Completed","2024-02-14T23:59:35","No","No","No","Internal"]
[null,null,null,34371,98556,"0_Tue Feb 13 2024 16:48:34 GMT+0800","2024-02-03T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Aft bilge well tank top to be cleaned and painted.","Miscellaneous","Eng. / Strg. Comp.","External Factors","","","","","Aft bilge well tank top cleaned and painted.","2024-03-04T23:59:35","","Completed","2024-02-13T23:59:35","No","No","No","Internal"]
[null,null,null,34372,76484,"0_Wed Feb 14 2024 21:25:01 GMT+0800","2024-02-03T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Aft bilge well tank top to be cleaned and painted.","Miscellaneous","Eng. / Strg. Comp.","External Factors","","","","","","2024-03-04T23:59:35","","Completed","2024-02-13T23:59:35","No","No","No","Internal"]
[null,null,null,34373,52700,"0_Wed Feb 14 2024 21:07:21 GMT+0800","2024-02-03T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","To fabricate stand for operating fire damper in AHU room","Accommodation","Eng. / Strg. Comp.","External Factors","","","","","A stand fabricated  for operating fire damper in AHU room","2024-03-04T23:59:35","","Completed","2024-02-13T23:59:35","No","No","No","Internal"]
[null,null,null,34374,20890,"0_Wed Feb 14 2024 21:12:45 GMT+0800","2024-02-03T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Incinerator waste oil tank man hole covers to be insulated with lagging.","Miscellaneous","Eng. / Strg. Comp.","External Factors","","","","","Incinerator waste oil tank man hole covers insulated with lagging.","2024-02-18T23:59:35","","Completed","2024-02-12T23:59:35","No","No","No","Internal"]
[null,null,null,34366,86017,"0_Wed Feb 14 2024 21:23:55 GMT+0800","2024-02-12T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ME jacket cooling FW inlet /outlet pipes near fwd aux blower , to be covered with insulation lagging.","Miscellaneous","Eng. / Strg. Comp.","External Factors","","","","","ME jacket coolig FW inlet/outlet pipes near fwd aux. blower covered with insulation lagging.","2024-03-04T23:59:35","","Completed","2024-02-12T23:59:35","No","No","No","Internal"]
[null,null,null,34363,77372,"123_Thu Feb 29 2024 08:03:58 GMT+0800","2024-02-22T23:59:35","Other","Ship Staff","Ship Staff Insp.","Hatch cover #6 Hydraulic Motor was found having minor leaks from the Motor bearing cover end.","Cargo Mach.","Cargo / Ballast Systems","External Factors","","","","","Hydraulic motor bearing cover end was opened, o rings renewed. Tried out, no leaks, operation satisfactory.","2024-03-10T23:59:35","","Completed","2024-02-28T23:59:35","No","No","No","Internal"]
[null,null,null,34364,40865,"0_Thu Feb 29 2024 08:05:17 GMT+0800","2024-02-24T23:59:35","Other","Ship Staff","Ship Staff Insp.","Hatch Cover #7 Hydraulic Motor was found having minor leaks from driven end.","Cargo Mach.","Cargo / Ballast Systems","External Factors","","","","","Motor overhauled , seal renewed. Tried out. No leaks. Operation good.","2024-03-10T23:59:35","","Completed","2024-02-27T23:59:35","No","No","No","Internal"]
[null,null,null,34365,24923,"123_Thu Feb 29 2024 17:40:03 GMT+0800","2024-02-26T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","While AE 3 running on normal sea load, found major cooling water leaking from attached LT pump.","E/R - Aux. Engine","Eng. / Strg. Comp.","External Factors","","","","","On inspection found small  hole on the suction side of pump casing. It was further observed after dismantling of the pump that the material around the suction side flange had thinned down. The casing repaired by welding. The pump all parts inspected found in order, The bearings, oil seal and mechanical seal renewed. The pump boxed back and pressure tested at 6 bar for one hour, no leakage observed. The pump fitted back in place and AE No. 3 cooling water opened and purging carried out.\n AE No. 3 tested, found working satisfactorily. The pump performance found satisfactory without any leakage, noise or vibration.","2024-03-01T23:59:35","","Completed","2024-02-27T23:59:35","No","No","No","Internal"]
[null,null,null,34353,22418,"123_Thu Feb 29 2024 18:37:44 GMT+0800","2024-02-29T23:59:35","Observation","Ship Staff","Ship Staff Insp.","LOW INSULATION FROM AE#2 LO PRIMING PUMP MOTOR.","E/R - Aux. Engine","Eng. / Strg. Comp.","External Factors","","","","","DG-2 L.O. PRIMING P/P MOTOR SHOWING ONE PHASE WINDING INSULATION VERY LOW. SAME OPENED UP FOR OVERHAULING. FOUND DRIVE END BEARING SEATING AREA COMPLETELY WORN OUT SO THE OUTER RACE OF THE BEARING WAS FREE IN THE BEARING HOUSING.  THIS IS THE REASON DUE TO WHICH THE STATOR AND ROTOR WINDING TOUCHING AND DEVELOPING LOW INSULATION.  VESSEL DOES NOT HAVE SPARE MOTOR SO THE SAME HOUSING REBUILDED BY WELDING AND USED. MOTOR TESTED FOUND WORKING SATISFACTORLIY. BUT STILL THIS PUMP WILL BE USED ONLY WHILE STARTING AE NO. 2. A NEW REQUISITION FOR MOTOR HAS BEEN RAISED.\nCHANGED ROTOR NDE & DE BEARINGS(6202ZZCM)\nCLEANED STATOR WINDINGS AND TESTED-FOUND WORKING SATISFACTORY","2024-03-31T23:59:35","PELA240036","Completed","2024-03-01T23:59:35","No","No","No","Internal"]
[null,null,null,34735,83854,"123_Fri Mar 15 2024 16:46:31 GMT+0800","2024-03-09T23:59:35","Critical Equipment","Ship Staff","Ship Staff Insp.","Lifeboat engine found not turning with starting motor once start activated. Engine not turning manually.","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","During routine testing of lifeboat engine, the engine failed to start with both the batteries. Engine was not even cranking when start switch was activated. After troubleshooting, it was found that engine was not even turning manually. Following this, the 3 fuel injectors were removed, tested for leaks but nothing abnormal was observed. Sump oil was drained, flushed and filled with fresh oil. Gear case was also opened up for inspection , but no abnormality/ leaks were found. Rocker arms were removed for all units, cleaned and fitted back, tappet clearance adjusted for all units. The engine was blown through after ensuring no oil in the cylinder head ( fuel injectors removed from their place) , the fuel lines was purged. Engine was given a start again with their injectors connected to the lines, but out of the engine, fuel injection was observed to be good, and no leaks/dripping was observed from fuel injectors. Engine was tried out multiple times after that and operation was found to be satisfactory. fuel tank outlet valve was found to be not holding, same was renewed. Return line was fitted with one ball valve.\nFuel injectors was again removed after a gap of almost a half day to check for any accumulating minor leaks. Engine was blown through. No oil leaks or accumulation was observed in the combustion space. Sump oil was checked. Found to be good and no increase/ mixing in the level was observed. Gear case was again opened for fuel pump, found minor traces of diesel oil  at the driving gear shaft seal area.\nOn 11th March 24, Fuel injectors were again removed from the engine & its return line was pressure tested with compressed air ( 5bar), with the injectors dipped in oil . No leak/ bubbles was observed from the injectors. Gear case was opened & inspected, no sign of leak.Sump oil checked,found ok. Fuel lines were purged, engine blown thru, no sign of oil ingress, injectors were boxed back up inside the engine. Engine was tried out. Found satisfactory","2024-03-15T23:59:35","PELA240043 RAISED FOR LIFEBOAT ENGINE SPARES ","Completed","2024-03-11T23:59:35","No","No","No","Internal"]
[null,null,null,34733,61330,"123_Wed Mar 13 2024 19:43:12 GMT+0800","2024-03-11T23:59:35","Other","Ship Staff","Ship Staff Insp.","FW LINE FROM FW HYDROPHORE TO ENGINE ROOM SERVICE ( NEAR FWD OF ME MANOEUVRING PLATFORM WAS FOUND TO BE LEAKING). ON CLOSER INSPECTION FOUND A PIN HOLE ON THE PIPE THAT HAD DEVELOPED OVER TIME, LEADING TO THE LEAK. ","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","External Factors","","","","","THE ENGINE ROOM FW SERVICE LINE WAS ISOLATED, THE PIPE WAS REMOVED FROM PLACE AND A NEW PIPE WAS FABRICATED IN ER WORKSHOP. NEW PIPE WAS FITTED AT THE PLACE WITH NEW GASKETS. LINE WAS PUT INTO USE. NO LEAKS FOUND. LINE PAINTED.","2024-03-31T23:59:35","","Completed","2024-03-11T23:59:35","No","No","No","Internal"]
[null,null,null,34734,77033,"123_Thu Mar 14 2024 18:59:26 GMT+0800","2024-03-14T23:59:35","Other","Ship Staff","Ship Staff Insp.","ACCOMODATION AC CONDENSOR SW OUTLET PIPE WAS FOUND WITH A MINOR LEAKAGE.","Accommodation","Eng. / Strg. Comp.","External Factors","","","","","SW LINE ISOLATED, REMOVED FROM PLACE AND REPAIRED IN WORKSHOP WITH WELDING. FITTED BACK WITH NEW GASKETS , TRIED OUT. NO LEAKS DETECTED.","2024-03-30T23:59:35","","Completed","2024-03-14T23:59:35","No","No","No","Internal"]
[null,null,null,34736,97235,"123_Sat Mar 30 2024 16:28:49 GMT+0800","2024-03-15T23:59:35","Defect","Ship Staff","Ship Staff Insp.","CARGO HOLD BILGE SUCTION COMMON VALVE ,LOCATED IN E/R, WAS FOUND TO BE NOT OPENING/CLOSING. ","E/R - Pipes/ valves & fittings","Cargo / Ballast Systems","External Factors","","","","","CARGO HOLD BILGE SUCTION COMMON VALVE GEAR WAS REMOVED FROM PLACE. WAS FOUND THAT THE VALVE GEAR CASING HAD DAMAGED/BROKEN. NEW VALVE GEAR WAS TAKEN FROM STORES AND PUT AT PLACE. OPERATION TRIED OUT, OPEN/CLOSE SATISFACTORY. ","2024-04-15T23:59:35","","Completed","2024-03-16T23:59:35","No","No","No","Internal"]
[null,null,null,34737,24033,"123_Sat Mar 30 2024 16:50:00 GMT+0800","2024-03-17T23:59:35","Other","Ship Staff","Ship Staff Insp.","BALLAST PUMP NO#1 SW SUCTION VALVE FOUND HARD TO OPERATE","E/R - Pipes/ valves & fittings","Cargo / Ballast Systems","External Factors","","","","","BALAST PUMP #1 SW SUCTION VALVE GEAR WAS REMOVED FROM PLACE AND OVREHAULED IN WORKSHOP. SPINDLE  SEATING GROOVE WAS FOUND TO BE INGRESSED WITH DIRT / GREASE . SAME WAS CLEANED AND LUBRICATED WITH FRESH GREASE. VALVE GEAR WAS PUT BACK IN PLACE. OPERATION FOUND SATISFACTORY.","2024-04-15T23:59:35","","Completed","2024-03-18T23:59:35","No","No","No","Internal"]
[null,null,null,34740,90311,"123_Sat Mar 30 2024 20:47:36 GMT+0800","2024-03-18T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Hatch cover #2 control box hydraulic hose was found with minor leak","Deck - Pipe / Fittings","Cargo / Ballast Systems","External Factors","","","","","Hatch cover #2 control box hydraulic hose was renewed with a spare hose ( 1 no). Operation was tried out, found satisfactory with no leaks.","2024-04-15T23:59:35","","Completed","2024-03-18T23:59:35","No","No","No","Internal"]
[null,null,null,34742,89211,"123_Sat Mar 30 2024 18:53:59 GMT+0800","2024-03-18T23:59:35","Defect","Ship Staff","Ship Staff Insp.","ME FO AUTOBACKWASH FILTER ACTUATOR MECHANISM WAS FOUND TO BE NOT OPERATIONAL. ","E/R - Aux. Mach.","Eng. / Strg. Comp.","External Factors","","","","","ME FO AUTOBACKWASH FILTER ACTUATOR WAS ISOLATED, AND REMOVED FROM PLACE. AFTER OVERHAULING FOUND THE O-RINGS OF ACTUATOR PISTON DAMAGED. NEW O-RINGS WAS USED AND THE ACTUATOR WAS CLEANED, LUBRICATED,BOXED UP, AND PUT IN PLACE.TRIED OUT, ACTUATOR FUNCTION SATISFACTORY.","2024-04-15T23:59:35","","Completed","2024-03-18T23:59:35","No","No","No","Internal"]
[null,null,null,34738,15479,"123_Sat Mar 30 2024 20:36:14 GMT+0800","2024-03-19T23:59:35","Defect","Ship Staff","Ship Staff Insp.","A CRACK WAS FOUND ON THE BULKHEAD OF NO #1 TST STBD ","Hull & Tanks","Cargo / Ballast Systems","Human Error,External Factors","","","","","CRACK IN THE NO 1 TST STBD SIDE WAS REPAIRED. BOTH SIDES OF THE CRACK, A HOLE WAS DRILLED TO ARREST THE CRACK, AND WAS FOLLOWED BY WELDING. CARRIED OUT NDT DYE PENETRANT TESTING FOR CRACK DETECTION AFTER THE REPAIR, NO CRACK DETECTED. VESSEL APPLIED FRESH COAT OF EPOXY AT THE REPAIRED AND SUROUNDING AREA.","2024-04-15T23:59:35","","Completed","2024-03-20T23:59:35","No","No","No","Internal"]
[null,null,null,34739,81124,"0_Sat Mar 30 2024 20:40:56 GMT+0800","2024-03-20T23:59:35","Defect","Ship Staff","Ship Staff Insp.","A CRACK WAS FOUND ON THE BULKHEAD OF NO 1 TST PORT ","Hull & Tanks","Cargo / Ballast Systems","External Factors","","","","","TWO HOLES WERE DRILLED AT THE EITHER ENDS OF THE CRACK TO PREVENT IT FROM SPREADING AND REDUCE THE STRESSES. THE CRACK WAS THEN REPAIRED BY WELDING. AFTER COMPLETION OF WELDING, NDT DYE PENETRANT TESTING WAS CARRIED OUT. NO CRACKS DETECTED. THE ADJACENT FRAMES WERE ALSO CHECKED FOR ANY SIMILAR DAMAGE. ALL FOUND SATISFACTORY. THE WELDED AREA WAS COVERED WITH 2 COAT EPOXY AND AFTER ADEQUATE CURING TIME THE TANK WAS BALLASTED. NO LEAKAGES FOUND INSIDE NO 1 CARGO HOLD.","2024-04-15T23:59:35","","Completed","2024-03-21T23:59:35","No","No","No","Internal"]
[null,null,null,34741,24662,"123_Sun Mar 31 2024 12:01:54 GMT+0800","2024-03-21T23:59:35","Defect,Other","Ship Staff","Ship Staff Insp.","HATCH COVER #6 CONTROL BOX FOUND HAVING A MINOR LEAK FROM ONE OF THE HYDRAULIC HOSE CONNECTION.","Deck - Pipe / Fittings","Cargo / Ballast Systems","External Factors","","","","","ON INSPECTION FOUND ONE CONNECTOR WITH DAMAGED O-RING. SAME RENEWED. OPERAION TRIED OUT. NO LEAK","2024-04-15T23:59:35","","Completed","2024-03-21T23:59:35","No","No","No","Internal"]
[null,null,null,34743,17151,"123_Sun Mar 31 2024 19:39:04 GMT+0800","2024-03-30T23:59:35","Defect","Ship Staff","Ship Staff Insp.","AE Jacket Cooler #1 ( Stbd) side, SW outlet pipe found leaking","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","External Factors","","","","","AE Jacket cooler #1 (Stbd) was immediately isolated, the pipe removed from place and taken to the workshop. The damaged portion of the pipe was cut off and a new length of pipe and flange was used to  refabricate the portion using welding. Pipe fitted back at place with new gaskets. Tried out. No leak, working satisfactory. Painted.","2024-04-15T23:59:35","","Completed","2024-03-31T23:59:35","No","No","No","Internal"]
[null,null,null,null,98052,"123_Thu Feb 29 2024 11:05:41 GMT+0800","2024-02-24T08:00:00","Defect","Ship Staff","Ship Staff Insp.","AE #2 Speed Switch got faulty resulting in the safeties and alarms, and remote start/start not working. AE#2 tried out from local and running good.","E/R - Aux. Engine","Eng. / Strg. Comp.","External Factors","","","","","Requisition received at Singapore. Pulse sensor and speed switch renewed. Alarms and trips tried out. Found working satisfactory.","2024-04-15T08:00:00","PELA240033","Completed","2024-04-01T08:00:00","No","No","No","Internal","Spare switch supplied in singapore."]
[null,null,null,null,79765,"123_Fri Apr 12 2024 11:16:58 GMT+0800","2024-04-02T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Hatch cover #4 Hydraulic Motor found leaking from the seal.","Cargo Mach.","Cargo / Ballast Systems","External Factors","","","","","Hatch cover #4 Hydraulic motor was opened up, on inspection found the seal of the bearing cover worn out. Same renewed with a new spare, O ring for the cover renewed as well. Hatch operation tried out, found satisfactory, no leakage detected. ","2024-04-30T08:00:00","","Completed","2024-04-02T08:00:00","No","No","No","Internal"]
[null,null,null,null,34221,"123_Sat Apr 13 2024 13:28:10 GMT+0800","2024-04-12T08:00:00","Defect","Ship Staff","Ship Staff Insp.","BWTS disinfectant pump outlet side piping found with minor leaks/salt traces.","E/R - Pipes/ valves & fittings","Cargo / Ballast Systems","External Factors","","","","","BWTS disinfectant pump outlet side was isolated. Pipe was removed from place and taken to the workshop, where a new pipe was fabricated. Pipe was pressure tested, found no leaks and then was painted. Same was fitted back at place with new gaskets. Line was put back to normal and was checked for leaks. Found satisfactory.","2024-04-30T08:00:00","","Completed","2024-04-12T08:00:00","No","No","No","Internal"]
[null,null,null,null,67537,"123_Sun Apr 14 2024 16:39:19 GMT+0800","2024-04-02T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Found AE #2 Jacket cooler SW inlet pipe with minor pin hole. To rectify/ fabricate.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","External Factors","","","","","Isolated the Jacket cooler, removed the SW inlet pipe, and taken to the workshop. New pipe fabricated, and painted. Same put at place with new gaskets. Cooler tried out, no leaks detected. Operation satisfactory.","2024-04-30T08:00:00","","Completed","2024-04-02T08:00:00","No","No","No","Internal"]
[null,null,null,null,32575,"123_Sun Apr 14 2024 16:50:42 GMT+0800","2024-03-28T08:00:00","Critical Equipment","Ship Staff","Ship Staff Insp.","TROUBLESHOOTING OF MSB 440V LOW INSULATION FROM ESB PANEL, VARIOUS BREAKERS.","Elect. Mach. & Equip.","Emgcy. Systems","External Factors","","","","","VESSEL RECEIVED MSB 440V LOW INSULATION FROM ESB PANEL FOLLOWING BREAKERS- \n(A)-E/R VENT FAN NO-1-MOTOR MEGGER TEST CARRIED OUT AND INSULATION VALUE FOUND TO BE 300MOHM.TRACES OF SALT RESIDUES FOUND FROM MULTIPLE ELECTRICAL & ELECTRONIC COMPONENTS BY CHECKING THE CIRCUIT DIAGRAM STEP BY STEP. CHANGED MAGNETIC CONTACTOR 42,E52A-3 AND 6-1 , CONTACTOR ROUTINES CARRIED OUT FOR MAGNETIC CONTACTOR 4RY , 4FY AND 88F. ALSO CHANGED THERMAL OVERLOAD RELAY OF MAGNETIC CONTACTOR 88F.ALSO MAINTENANCE CARRIED OUT FOR AUTO-TRANSFORMER-CLEANED WINDINGS AND APPLIED VARNISH AND KEPT FOR WARMING UP FOR 3 HRS BY CARGO LIGHTS. MEGGER TEST CARRIED OUT AND IR VALUE FOUND TO BE 35 MOHM. ALSO CHANGED MAIN MCCB ON ESB PANEL AS IT WAS ALSO A CAUSE OF LOW INSULATION. FUNCTION TEST CARRIED OUT AND E/R VENT FAN NO-1 FOUND WORKING SATISFACTORY WITHOUT ANY DROP IN IR VALUE.   \n(B)-E/G ROOM EXH FAN-MOTOR MEGGER TEST CARRIED OUT AND INSULATION VALUE FOUND TO BE 300MOHM.TRACES OF SALT RESIDUES FOUND ON OVERLOAD THERMAL RELAY COIL AT R & T PHASES. SAME WAS CLEANED AND TESTED BUT DROP IN IR VALUE WAS OBSERVED SO THE WHOLE ASSEMBLY OF MAGNETIC CONTACTOR AND THERMAL OVERLOAD RELAY WAS RENEWED. AGAIN AFTER TESTING IR VALUE DROP WAS OBSERVED AFTER THIS IN THE CIRCUIT WHICH WAS DUE TO SAFETY MODULE ESM-1153-CLEANED MODULE WITH CRC ELECTRO CLEAN AND TESTED BUT DROP WAS OBSERVED IN IR VALUE SO ESM-1153 WAS RENEWED. FUNCTION TEST CARRIED OUT AND FAN FOUND WORKING SATISFACTORY WITHOUT ANY DROP IN IR VALUE. \n(C)- EMERGNCY FIRE P/P-TRACED LOW INSULATION FROM THE OUTPUT TERMINALS OF MCCB  AND ROUTINES CARRIED-CLEANED THE TERMINALS AND FUNCTION TEST CARRIED OUT-NO DROP OF IR VALUE WAS OBSERVED.\n(D)-EMERGENCY USE TRANSFORMER NO-1-LOW INSULATION WAS OBSERVED FROM THIS TRANSFORMER .DISCONNECTED THE CIRCUIT AND REMOVED THE TRANSFORMER.MEGGER TEST CARRIED OUT AND IR VALUE FOUND TO BE 1 MOHM.CLEANED THE WINDINGS AND APPLIED VARNISH, KEPT FOR WARMING UP FOR 3 HRS BY USING CARGO LIGHT.ASSEMBLED BACK AND MEGGER TEST CARRIED OUT-IR VALUE CAME TO 100MOHM.","2024-04-30T08:00:00","","Completed","2024-03-31T08:00:00","No","No","No","Internal"]
[null,null,null,null,94250,"123_Tue Apr 30 2024 14:12:57 GMT+0800","2024-04-18T08:00:00","Defect","Ship Staff","Ship Staff Insp.","BWTS disinfectant liquid pipe section was found with a minor leak","E/R - Pipes/ valves & fittings","Cargo / Ballast Systems","External Factors","","","","","BWTS disinfectant liquid pipe section was isolated, removed from place and a new pipe was fabricated in the workshop. Same fitted back and tried out. No leaks.","2024-05-15T08:00:00","","Completed","2024-04-18T08:00:00","No","No","No","Internal"]
[null,null,null,null,27313,"0_Tue Apr 30 2024 14:21:51 GMT+0800","2024-04-27T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Cargo hold bilge line suction valve found not operating manually.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","External Factors","","","","","The line was isolated, the valve gear was removed and upon inspection it was found that the valve spindle had broken.  The spindle was repaired using welding, the valve was cleaned and eased up. Valve boxed up and put at place. Tried out found working satisfactory.","2024-05-15T08:00:00","","Completed","2024-04-27T08:00:00","No","No","No","Internal"]
[null,null,null,null,41981,"123_Tue Apr 30 2024 19:35:03 GMT+0800","2024-04-22T08:00:00","Defect","Ship Staff","Ship Staff Insp.","OWS outlet pipe section developed a hole","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","External Factors","","","","","OWS pipe section was isolated, seal removed, and a new pipe was fabricated in the workshop and pressure tested. Found ok. Same installed at the OWS section. New seal used. Satisfactory. Photos attached.","2024-05-15T08:00:00","","Completed","2024-04-22T08:00:00","No","No","No","Internal"]
[null,null,null,null,25321,"123_Wed Nov 15 2023 20:41:46 GMT+0800","2024-01-02T08:00:00","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","14 in number Bobby hatch embarkation steps to replace with new shore fabricated steps, location to be confirmed by master after checking all the steps.","Deck - Pipe / Fittings","Cargo / Ballast Systems","External Factors","","","","","Cropped & replaced new steps of bobby hatch embarkation steps.","2024-05-15T08:00:00","","Completed","2024-04-26T08:00:00","No","No","No","Internal","The job to be completed in next ballast voyage"]

{"sheet":"Calc","index":2,"n_rows":28,"n_cols":12,"rows_kept":28,"cut":false,"hidden":true,"merged":[]}
["Def_type","Def_cause","Equipments","VIQrefno","Observer_code"]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,"Dim itemSele As Long"]
[null,null,null,null,null,null,null,null,null,null,null,"   dim startRow as integer"]
[null,null,null,null,null,null,null,null,null,null,null,"   startRow=1"]
[null,null,null,null,null,null,null,null,null,null,null,"        For itemSele = 0 To ListBox1.ListCount - 1"]
[null,null,null,null,null,null,null,null,null,null,null,"        If ListBox1.Selected(itemSele) = True Then"]
[null,null,null,null,null,null,null,null,null,null,null,"        Worksheets(\"WorksheetName\").Range(\"A\" & startRow).Value = ListBox1.List(itemSele)"]
[null,null,null,null,null,null,null,null,null,null,null,"        startRow = startRow + 1"]
[null,null,null,null,null,null,null,null,null,null,null,"        End If"]
[null,null,null,null,null,null,null,null,null,null,null,"        Next"]
[null,null,null,null,null,null,null,null,null,null,null,"Dim LastRowA As String"]
[null,null,null,null,null,null,null,null,null,null,null,"        Dim itemSele As Long"]
[null,null,null,null,null,null,null,null,null,null,null,"       Dim startRow as integer"]
[null,null,null,null,null,null,null,null,null,null,null,"        LastRowA = ActiveSheet.Cells(Rows.count, \"A\").End(xlUp).row"]
[null,null,null,null,null,null,null,null,null,null,null,"        startQue = 0"]
[null,null,null,null,null,null,null,null,null,null,null,"        For itemSele = 0 To ListBox1.ListCount - 1"]
[null,null,null,null,null,null,null,null,null,null,null,"        For startRow = 1 To LastRowA"]
[null,null,null,null,null,null,null,null,null,null,null,"        If Worksheets(\"WorksheetName\").Range(\"A\" & startRow).Value = ListBox1.List(itemSele) Then"]
[null,null,null,null,null,null,null,null,null,null,null,"        ListBox1.Selected(itemSele) = True"]
[null,null,null,null,null,null,null,null,null,null,null,"        Exit For"]
[null,null,null,null,null,null,null,null,null,null,null,"        End If"]
[null,null,null,null,null,null,null,null,null,null,null,"        Next j"]
[null,null,null,null,null,null,null,null,null,null,null,"        Next"]
[null,null,null,null,null,null,null,null,null,null,null,"        End If"]

{"sheet":"Areaofobs","index":3,"n_rows":17,"n_cols":2,"rows_kept":17,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Cargo / Ballast Systems",11]
["Cert. & Docu.",2]
["Communication",6]
["Crew Management",3]
["Emgcy. Systems",13]
["Eng. / Strg. Comp.",14]
["General Appearance",15]
["Ice Opns.",17]
["ISM Related",7]
["ISPS Related",10]
["MARPOL Related",9]
["MLC Related",4]
["Mooring",12]
["Navigation",5]
["Safety / LSA / FFA",8]
["Structural Condn. / WT integrity ",16]

{"sheet":"Vessel_type","index":4,"n_rows":1,"n_cols":2,"rows_kept":1,"cut":false,"hidden":true,"merged":[]}
["Vessel_type","ID"]

{"sheet":"Deficiency_type","index":5,"n_rows":8,"n_cols":3,"rows_kept":8,"cut":false,"hidden":true,"merged":[]}
["TITLE","Type of deficiency_description","ID"]
["Breakdown",null,6]
["Critical Equipment",null,4]
["Defect",null,1]
["Guarantee Claim",null,8]
["Non Conformity",null,2]
["Observation",null,3]
["Other",null,7]

{"sheet":"VIQrefno","index":6,"n_rows":1,"n_cols":3,"rows_kept":1,"cut":false,"hidden":true,"merged":[]}
["VIQ_ref_no","Risk Value of observation","ID"]

{"sheet":"Equipment_list","index":7,"n_rows":28,"n_cols":3,"rows_kept":28,"cut":false,"hidden":true,"merged":[]}
["TITLE","Equipment_list_description","ID"]
["Accommodation",null,12]
["Cargo Mach.",null,13]
["Critical Equip.",null,16]
["Deck - Machinery",null,18]
["Deck - Mooring Machinery",null,15]
["Deck - Pipe / Fittings",null,20]
["Documentation",null,21]
["E/R - Air Comp.",null,8]
["E/R - Aux. Engine",null,4]
["E/R - Aux. Mach.",null,7]
["E/R - Boiler",null,5]
["E/R - Main Engine",null,3]
["E/R - Pipes/ valves & fittings",null,9]
["E/R - Pumps",null,32]
["E/R - Purifier",null,6]
["Elect. Mach. & Equip.",null,10]
["Hull & Tanks",null,19]
["Inert Gas",null,14]
["LSA / FFA",null,17]
["Miscellaneous",null,22]
["Navigation - DGPS / EPFS / AIS",null,28]
["Navigation - ECDIS",null,25]
["Navigation - Echo Sounder / Speed Log",null,26]
["Navigation - GMDSS & Communication",null,23]
["Navigation - Others",null,11]
["Navigation - RADAR",null,24]
["Navigation - VDR / BNWAS",null,30]

{"sheet":"PSC_MOU","index":8,"n_rows":11,"n_cols":3,"rows_kept":11,"cut":false,"hidden":true,"merged":[]}
["TITLE","PSC_MOU_description","ID"]
["Asia and the Pacific",null,2]
["Caribbean",null,4]
["Europe and the North Atlantic",null,1]
["Latin America",null,3]
["The Black Sea region",null,6]
["The Indian Ocean",null,8]
["The Mediterranean",null,7]
["The Riyadh MoU",null,9]
["USCG",null,10]
["West and Central Africa",null,5]

{"sheet":"Inspection_type","index":9,"n_rows":13,"n_cols":2,"rows_kept":13,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Bunkering Audit",14]
["Cargo Audit",17]
["Engineering Audit",16]
["ISM Audit",2]
["ISPS Audit",3]
["IT Audit",10]
["MLC Audit",1]
["Mooring Audit",9]
["Nav Audit / Verification",8]
["Onboard Training",18]
["Ship Staff Insp.",15]
["Suptd. Insp.",13]

{"sheet":"Deficiency_Cause","index":10,"n_rows":8,"n_cols":3,"rows_kept":8,"cut":false,"hidden":true,"merged":[]}
["TITLE","Deficiency_Cause_description","ID"]
["Behaviour Based",null,1]
["Equipment Related",null,4]
["External Factors",null,5]
["Human Error",null,7]
["Inappropriate Procedure",null,8]
["Industry Issue",null,6]
["Knowledge Based",null,3]

{"sheet":"Observer_code","index":11,"n_rows":3,"n_cols":3,"rows_kept":3,"cut":false,"hidden":true,"merged":[]}
["TITLE","Observer_code_description","ID"]
["Owner / Marine / Tech. Suptd.",null,3]
["Ship Staff",null,2]

{"sheet":"Status_code","index":12,"n_rows":6,"n_cols":3,"rows_kept":6,"cut":false,"hidden":true,"merged":[]}
["TITLE","Status_code_description","ID"]
["Completed",null,6]
["Deferred to D D",null,5]
["In progress",null,3]
["Not Started",null,2]
["Waiting spare",null,4]

{"sheet":"PSC_ref_no","index":13,"n_rows":19,"n_cols":2,"rows_kept":19,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Alarms",9]
["Cargo operations including equipment",7]
["Certificates & Documentation",2]
["Dangerous Goods",13]
["Emergency Systems",5]
["Fire safety",8]
["ISM",16]
["ISPS",17]
["Life saving appliances",12]
["MLC, 2006",18]
["Other",19]
["Pollution Prevention",15]
["Propulsion and auxiliary machinery",14]
["Radio communication",6]
["Safety of Navigation",11]
["Structural condition",3]
["Water/Weathertight condition",4]
["Working and Living Conditions",10]

{"sheet":"Risk_value_of_obs","index":14,"n_rows":1,"n_cols":2,"rows_kept":1,"cut":false,"hidden":true,"merged":[]}
["Risk Value of observation","ID"]

{"sheet":"Year","index":15,"n_rows":18,"n_cols":1,"rows_kept":18,"cut":false,"hidden":true,"merged":[]}
["Year"]
[2014]
[2015]
[2016]
[2017]
[2018]
[2019]
[2020]
[2021]
[2022]
[2023]
[2024]
[2025]
[2026]
[2027]
[2028]
[2029]
[2030]

{"sheet":"Month","index":16,"n_rows":13,"n_cols":1,"rows_kept":13,"cut":false,"hidden":true,"merged":[]}
["Month"]
["Jan"]
["Feb"]
["Mar"]
["Apr"]
["May"]
["Jun"]
["Jul"]
["Aug"]
["Sep"]
["Oct"]
["Nov"]
["Dec"]

{"sheet":"Date_","index":17,"n_rows":32,"n_cols":1,"rows_kept":32,"cut":false,"hidden":true,"merged":[]}
["Date"]
["01"]
["02"]
["03"]
["04"]
["05"]
["06"]
["07"]
["08"]
["09"]
[10]
[11]
[12]
[13]
[14]
[15]
[16]
[17]
[18]
[19]
[20]
[21]
[22]
[23]
[24]
[25]
[26]
[27]
[28]
[29]
[30]
[31]

{"sheet":"Sheet1","index":18,"n_rows":24,"n_cols":6,"rows_kept":24,"cut":false,"hidden":true,"merged":[]}
[]
[null,"ID","E",null,"Date Recorded",1]
[null,"UNIQUE ID","F",null,"Type of Deficiency",2]
[1,"Date Recorded","G",null,"Observer code",3]
["ignore","Vessel Type","H",null,"Type of Inspection",4]
[null,"Internal / External","I",null,"Description of Deficiency",5]
[null,"Drydock","J",null,"Equipment Categories",6]
[null,"Information Sharing","K",null,"Area of Observation",7]
[null,"Critical_item","L",null,"Deficiency Cause",8]
[null,"Deficiency Type","M",null,"VIQ Ref Number",9]
[null,"Deficiency Cause","N",null,"Risk Value of Obs",10]
[null,"Inspection Type","O",null,"PSC Ref Number",11]
[null,"Equipments","P",null,"PSC MOU ID",12]
[null,"VIQ Reference Number","Q",null,"Action Taken or Required",13]
[null,"Risk Value of the observation","R",null,"Target Date",14]
[null,"PSC Reference Number","S",null,"PO Ref No.",15]
[null,"PSC MOU","T",null,"Status Code",16]
[null,"Observer Code","U",null,"Date Completed",17]
[null,"Target Date","V",null,"Drydock",18]
[null,"Status Code","W",null,"Info Sharing",19]
[null,"Description of Deficiency","X",null,"Critical Item Flag",20]
[null,"Action taken / required","Y",null,"Audit Type",21]
[null,"PO ref no","Z"]
[null,"Date completed","AA"]

{"sheet":"Ship_information","index":19,"n_rows":2,"n_cols":4,"rows_kept":2,"cut":false,"hidden":true,"merged":[]}
["Ship_ID","Ship_Name","FILE_NAME","Export_Date"]
["123","PELAGOS (03-04-2024)","123_1712110141317.xlsm","2024-05-01 00:05:40"]

{"sheet":"External_Deficiency_type","index":20,"n_rows":5,"n_cols":3,"rows_kept":5,"cut":false,"hidden":true,"merged":[]}
["TITLE","Type of deficiency_description","ID"]
["Condn of Class / Memo",null,5]
["Defect",null,1]
["Non Conformity",null,2]
["Observation",null,3]

{"sheet":"External_Inspection_type","index":21,"n_rows":11,"n_cols":2,"rows_kept":11,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Cargo Audit",17]
["Flag State Insp.",5]
["ISM Audit",2]
["ISPS Audit",3]
["MLC Audit",1]
["Nav Audit / Verification",8]
["OM Insp. (Eg. SIRE / CDI etc.)",6]
["Others (Eg. Insurance etc.)",12]
["PSC Inspection",4]
["Terminal Insp.",11]

{"sheet":"External_Observer_code","index":22,"n_rows":7,"n_cols":3,"rows_kept":7,"cut":false,"hidden":true,"merged":[]}
["TITLE","Observer_code_description","ID"]
["Class Surveyor",null,4]
["FSC Inspector",null,5]
["Others (Eg. Insurance etc.)",null,9]
["PSC Insp.",null,6]
["SIRE / CDI Insp.",null,8]
["Terminal Insp.",null,7]

{"sheet":"Sheet Version","index":23,"n_rows":2,"n_cols":2,"rows_kept":2,"cut":false,"hidden":true,"merged":[]}
["Version","Title"]
["2.0","Version 2.0"]