{"text_format":"1","workbook":"xlsx","n_sheets":24,"sheets":["Mainsheet","Completed","Calc","Areaofobs","Vessel_type","Deficiency_type","VIQrefno","Equipment_list","PSC_MOU","Inspection_type","Deficiency_Cause","Observer_code","Status_code","PSC_ref_no","Risk_value_of_obs","Year","Month","Date_","Sheet1","Ship_information","External_Deficiency_type","External_Inspection_type","External_Observer_code","Sheet Version"],"not_rendered":{"charts":0,"images":1,"macros":1,"external_links":0,"defined_names":12,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Mainsheet","index":0,"n_rows":56,"n_cols":28,"rows_kept":56,"cut":false,"hidden":false,"merged":[[10,8,10,9],[10,12,10,13],[12,6,12,27],[8,6,8,27]]}
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,"Defect - Damage Monitoring Sheet"]
[]
[null,null,null,null,null,null,null,"Date of Report","13-May-2024",null,null,"Ship Name","DHT LOTUS (04-03-2024)"]
[]
[null,null,null,null,null,null,"VERSION : 2.0"]
[]
[]
[]
[null,null,null,"ID","SHIPSIDE UNIQUEID","UNIQUE ID","Date Recorded","Type of Deficiency","Observer code","Type of Inspection","Description of Deficiency","Equipment Categories","Area of Observation","Deficiency Cause","VIQ Ref Number","Risk Value of Obs","PSC Ref Number","PSC MOU ID","Action Taken or Required","Target Date","PO Ref No.","Status Code","Date Completed","Drydock","Info Sharing","Critical Item","Audit Type","Superintendent Remarks"]
[null,null,null,null,97699,"27_Sun Sep 17 2023 14:39:06 GMT+0800","2023-08-24T08:00:00","Defect","Ship Staff","Ship Staff Insp.","ME # 7 unit JCW outlet valve not holding","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Vessel has spare valve, same will be replaced at a suitable opportunity. The operation of main engine unit no.7 is satisfactory without any leakages of jacket water.","2024-06-30T08:00:00","","Not Started",null,"No","No","No","Internal"]
[null,null,null,null,98889,"27_Sat Sep 16 2023 08:40:25 GMT+0800","2023-09-01T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Galley AC unit cooler not working","Elect. Mach. & Equip.","MLC Related","Equipment Related","","","","","Spares received, job planned.","2024-05-30T08:00:00","DLOT240004","In progress",null,"No","No","No","Internal"]
[null,null,null,null,15285,"0_Sat Sep 16 2023 19:53:52 GMT+0800","2023-09-01T08:00:00","Defect","Ship Staff","Ship Staff Insp.","EGCS # 3 SW pump motor drive end bearing making noise","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","Carried out greasing routines for driving and non driving end bearing, under observation, EGCS system have 3 pumps in total, Pump no.1 and no.2 are working is satisfactory condition.","2024-06-30T08:00:00","","In progress",null,"No","No","No","Internal"]
[null,null,null,null,24520,"0_Sun Sep 17 2023 07:47:26 GMT+0800","2023-09-09T08:00:00","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Aircon to install for the EGCS supply pump VFD starter panel.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","","2024-05-30T08:00:00","","In progress",null,"No","No","No","Internal"]
[null,null,null,null,91055,"27_Sat Oct 21 2023 07:38:16 GMT+0800","2023-10-19T08:00:00","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Few Hydraulic box covers have knife edges due to corrosion while some need their channels to be built up","Deck - Pipe / Fittings","General Appearance","External Factors","","","","","Wasted covers to be brought to engine room workshop for repairs one by one. There is no observed ingress of water, temporary repairs with duct tape carried out around the surface to avoid any ingress of water.","2024-05-30T08:00:00","","In progress",null,"No","No","No","Internal"]
[null,null,null,null,53270,"0_Sun Nov 19 2023 07:26:33 GMT+0800","2023-11-15T08:00:00","Defect","Ship Staff","Ship Staff Insp.","# 3 D/G exhaust leakage from uptake at various locations","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","# 3 D/G exhaust leakage from uptake to be inspected & rectified. Section by section is checked for any leakages, the leakage is within acceptable limit.","2024-06-30T08:00:00","","In progress",null,"No","No","No","Internal"]
[null,null,null,null,67964,"27_Mon Dec 04 2023 14:21:11 GMT+0800","2023-11-27T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Stern tube LO flow meter found not displaying flow rate.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","Flowmeter need to be replaced with new spare. Stern tube lube oil piping system is operational, with temperatures and pressure within normal range.","2024-08-30T08:00:00","DLOT240035","Waiting spare",null,"No","No","No","Internal"]
[null,null,null,null,41354,"0_Mon Dec 18 2023 16:53:37 GMT+0800","2023-12-05T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Stbd provison crane slewing circuit balance valve found leaking.","Deck - Machinery","Eng. / Strg. Comp.","Equipment Related","","","","","Stbd provision crane slewing circuit balance valve found leaking. RO - DLOT230305 raised. Temporary leak is arrested by cold work.","2024-05-30T08:00:00","","In progress",null,"No","No","No","Internal"]
[null,null,null,null,76254,"27_Tue Jan 30 2024 01:00:56 GMT+0800","2024-01-02T08:00:00","Observation","Owner / Marine / Tech. Suptd.","Ship Staff Insp.","Port and Stbd windlass upper brake - wastage","Deck - Machinery","Mooring","Equipment Related","10.3","Medium","","","P.O raised - awaiting supply","2024-06-08T08:00:00","DLOT240025","Waiting spare",null,"No","No","No","Internal"]
[null,null,null,null,59588,"27_Sat Jan 27 2024 22:31:13 GMT+0800","2024-01-03T08:00:00","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","LT cooler no.2 sea water pipe is leaking, same to be rectified.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","LT cooler need to be isolated and sea water leak to be arrested. There are two leaks, one is at the inlet flange and another is at welding seam for overboard line, we need to isolate cooler and shut down overboard valve. The leak is arrested by temporary cold work, permanent job will be carried out at suitable opportunity.","2024-06-30T08:00:00","","In progress",null,"No","No","No","Internal"]
[null,null,null,null,44165,"27_Sat Jan 27 2024 18:56:01 GMT+0800","2024-01-03T08:00:00","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Main engine air cooler feed water preheater air side gasket is leaking, the moisture from scavenge air is coming out from preheater end flange. ","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","The gasket for the flange to be replaced, Vessel need to be a anchorage  to change the Air cooler feed water heater gasket. The Air leak is minimum and does not hamper the loss of scavenge pressure.","2024-08-30T08:00:00","","Not Started",null,"No","No","No","Internal"]
[null,null,null,null,71569,"27_Sat Jan 27 2024 19:08:07 GMT+0800","2024-01-03T08:00:00","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","The line for Air cooler feed water preheater is having a expansion/flexible pipe which is having a leak.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","New expansion/flexible pipe to be procured and to be replaced with the defective one. Currently the leak from expansion pipe connection is stopped, ","2024-06-30T08:00:00","DLOT240033","In progress",null,"No","No","No","Internal"]
[null,null,null,null,62519,"27_Sat Jan 27 2024 22:33:41 GMT+0800","2024-01-22T08:00:00","Observation","Ship Staff","Ship Staff Insp.","Vacuum condenser end cover are leaking of sea water.","Cargo Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","End covers for vacuum condenser to be overhauled and gasket to be renewed. The leak is minimal and does not hamper the condenser operation/efficiency.","2024-08-30T08:00:00","DLOT240034","Waiting spare",null,"No","No","No","Internal"]
[null,null,null,null,24241,"27_Fri Feb 02 2024 19:31:47 GMT+0800","2024-01-30T08:00:00","Breakdown","Ship Staff","Ship Staff Insp.","Aux feed pump no.2 is not developing enough pressure and drawing more current.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","","","","","Pump rotating parts are weared down, parts to be replaced. The other pump Aux feed pump no.1 is operational.","2024-05-30T08:00:00","DLOT240010","In progress",null,"No","No","No","Internal"]
[null,null,null,null,83091,"27_Fri Feb 02 2024 19:25:00 GMT+0800","2024-01-31T08:00:00","Breakdown","Ship Staff","Ship Staff Insp.","TG condenser cooling sea water pump no.1 top volute cover is corroded and wasted, making it difficult to fit mouth ring.","E/R - Aux. Mach.,E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","","","","","New top volute cover is on order. The other TG condenser cooling sea water pump no.2 is operational and can be put into use when required.","2024-08-30T08:00:00","DLOT240017","Waiting spare",null,"No","No","No","Internal"]
[null,null,null,null,66264,"27_Fri Feb 02 2024 19:36:39 GMT+0800","2024-01-31T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Aux engine fuel oil feeder pump and booster pump are not in standby mode.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","","","","","Timer relay is faulty. Both the pumps are working satisfactory in manual mode.","2024-08-30T08:00:00","DLOT240022","Waiting spare",null,"No","No","No","Internal"]
[null,null,null,null,80306,"27_Thu Mar 14 2024 16:25:08 GMT+0800","2024-03-01T08:00:00","Observation","Ship Staff","Ship Staff Insp.","ODME annual servicing due March 2024 - ODME Slop recirculation valve CAV 188 actuator leaking and with soft repair.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","6.13","Low","","","1. Company informed awaiting confirmation and PO raised.\n2. Annual test carried out onboard for certification and records submitted.\n3. Awaiting shore certificate","2024-05-31T08:00:00","DLOT240045 - NAKAKITA ACTUATOR FOR ODME SLOP RECIRCULATION VALVE @SINGAPORE","In progress",null,"No","No","No","Internal"]
[null,null,null,null,31965,"27_Thu Mar 14 2024 23:05:52 GMT+0800","2024-03-01T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Main engine fuel oil control unit (FCU) is having an alarm for mixing column low level, suspect the level sensor is faulty. ","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","The level sensor to be replaced with new spare. The job can be carried out with Main engine in stopped condition either in port or at anchorage.","2024-08-30T08:00:00","DLOT240062","Not Started",null,"No","No","No","Internal"]
[null,null,null,null,91316,"27_Thu Mar 14 2024 23:08:14 GMT+0800","2024-03-01T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Main engine lube oil purifier heater no.1 steam inlet valve operating wheel is broken","E/R - Purifier","Eng. / Strg. Comp.","Equipment Related","","","","","Heater inlet valve to be replaced with new spare.","2024-05-30T08:00:00","","Not Started",null,"No","No","No","Internal"]
[null,null,null,null,36044,"27_Thu Mar 14 2024 23:15:18 GMT+0800","2024-03-01T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Under piston drain dirty oil tank port side drain valve is leaking, making the vent line pressurized to some extent.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Valve to be replaced with new spare.","2024-05-30T08:00:00","","Not Started",null,"No","No","No","Internal"]
[null,null,null,34662,53640,"27_Thu Mar 14 2024 23:17:46 GMT+0800","2024-03-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","EGB soot blowers sealing air fan line is broken and not operational.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Soot blowers air sealing line to be made clear of any debris, some pipe sections to be fabricated and sealing air fan to be made operational.","2024-05-30T23:59:35","","Not Started",null,"No","No","No","Internal"]
[null,null,null,null,44392,"27_Thu Mar 14 2024 23:23:54 GMT+0800","2024-03-01T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Flexible rubber pipe connection for cooling water inlet and outlet for Aux engine 1 and 2 are found to be in poor condition, with cracks visible.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Flexible rubber pipe connection for cooling water to be replaced with new spare.  Total 4 pcs in total, out of which 1 pc for Aux engine no.2 inlet rubber pipe connection is replaced with new spare.","2024-05-30T08:00:00","DLOT240041","In progress",null,"No","No","No","Internal"]
[null,null,null,null,89225,"27_Thu Mar 14 2024 23:11:44 GMT+0800","2024-03-01T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Sewage treatment plant discharge pump outlet valve is broken.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Valve to be replaced with new/reconditioned spare.","2024-05-30T08:00:00","","In progress",null,"No","No","No","Internal"]
[null,null,null,null,25734,"27_Thu Mar 14 2024 23:29:34 GMT+0800","2024-03-01T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Steam pipe going for Engine room steam consumption 7.7k line, pipe flange after the reducer is found to be leaking, location is above TG vacuum pump on 3rd deck, 6metres high above TG vacuum pump.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Pipe flange connection overhauled at USA, gasket renewed, the leak still exist, suspect the flange is having dent/cut, need to remove end to end flange connection of the pipe and carry out the repairs accordingly. The job require scaffolding staging.","2024-06-30T08:00:00","","In progress",null,"No","No","No","Internal"]
[null,null,null,null,18048,"27_Fri Mar 15 2024 00:32:49 GMT+0800","2024-03-01T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Slop S WSU repeater  - temperature display in CCR not working.","","Cargo / Ballast Systems","Equipment Related","8.40","High","","","Technician attended at last call Singapore on 02 Jan 2024 & as per him the system is obsolete & no more spares available with maker for renewal. Awaiting further instruction.","2024-05-31T08:00:00","","In progress",null,"No","No","No","Internal"]
[null,null,null,null,71516,"27_Fri Mar 15 2024 00:57:00 GMT+0800","2024-03-01T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Several railings Wasted.","","Safety / LSA / FFA","Equipment Related","11.5","Medium","","","Vessel in Loaded condition and planned during ballast passage.","2024-05-31T08:00:00","","In progress",null,"No","No","No","Internal"]
[null,null,null,null,42274,"27_Fri Mar 15 2024 01:04:20 GMT+0800","2024-03-01T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Lights bracket around accommodation rusted, wasted and lights defective. ","Accommodation","Safety / LSA / FFA","Equipment Related","11.11","Very High","","","De-rusting, painting and renewal of lights in progress. Lights near Accommodation Port and Stbd replaced with new fabricated fitting and enclosure. Out of 4, 2 are completed.","2024-05-30T08:00:00","","In progress",null,"No","No","No","Internal"]
[null,null,null,null,30507,"27_Fri Mar 15 2024 01:09:29 GMT+0800","2024-03-01T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Paint room Weathertight door edges wastage.","Miscellaneous","Structural Condn. / WT integrity ","Equipment Related","11.6","Medium","","","Cold repair done, need to carry out permanent repair using hot work at suitable opportunity..","2024-06-30T08:00:00","","Not Started",null,"No","No","No","Internal"]
[null,null,null,null,15177,"27_Fri Mar 15 2024 15:26:21 GMT+0800","2024-03-01T08:00:00","Defect","Ship Staff","Ship Staff Insp.","HFO transfer pump mech seal is found to be leaking.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","","","","","HFO transfer pump mech seal to be replaced with new spare.","2024-08-30T08:00:00","DLOT240061","Waiting spare",null,"No","No","No","Internal"]
[null,null,null,null,87924,"27_Fri Mar 15 2024 15:28:01 GMT+0800","2024-03-01T08:00:00","Defect","Ship Staff","Ship Staff Insp.","EGCS SOX scrubber pump no.2 is leaking from mech seal","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","","","","","EGCS SOX scrubber sea water pump no.2 mech seal is found to be leaking, same to be replaced with new spare mech seal.","2024-05-30T08:00:00","","Not Started",null,"No","No","No","Internal"]
[null,null,null,null,37090,"27_Fri Mar 15 2024 15:31:34 GMT+0800","2024-03-01T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Both Air cooler feed water preheater is found to be leaking of feed water.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","The Feed water preheater fitted inside Main engine Air coolers is found to be leaking of feed water. The preheater to be removed and pressure tested to locate the leak and rectify accordingly. The open section at the Air cooler to be blanked and feed water to be by pass to the heater till the preheater are fitted back in.","2024-05-30T08:00:00","","In progress",null,"No","No","No","Internal"]
[null,null,null,null,89252,"27_Fri Mar 15 2024 15:47:45 GMT+0800","2024-03-01T08:00:00","Defect","Ship Staff","Ship Staff Insp.","IG fan no.1 ammeter is faulty.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Ammeter to be replaced with new spare.","2024-05-30T08:00:00","DLOT240042","Waiting spare",null,"No","No","No","Internal"]
[null,null,null,34680,52403,"27_Fri Mar 15 2024 15:51:13 GMT+0800","2024-03-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","TG condenser cooling sea water pump discharge valve is leaking through flange gasket","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Flange gasket to be renewed. The leak is visible by stain marks. The valve size is 350A.","2024-05-31T23:59:35","","Not Started",null,"No","No","No","Internal"]
[null,null,null,34681,84864,"27_Fri Mar 15 2024 15:53:55 GMT+0800","2024-03-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Vacuum condenser by pass valve near Vacuum pump is leaking through flange gasket.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","The flange gasket for the valve is leaking, valve size is 450A. The leak is visible because of stain marks.","2024-05-31T23:59:35","","Not Started",null,"No","No","No","Internal"]
[null,null,null,34682,16515,"27_Fri Mar 15 2024 16:02:35 GMT+0800","2024-03-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Vacuum condenser out line elbow pipe connection flange gasket is leaking.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Pipe to be disconnected and flange gasket to be renewed, pipe size is 450A. The leak is visible because of stain marks.","2024-05-31T23:59:35","","Not Started",null,"No","No","No","Internal"]
[null,null,null,null,38686,"27_Thu Mar 14 2024 23:54:18 GMT+0800","2024-03-01T08:00:00","Observation","Ship Staff","Ship Staff Insp.","Ballast gauges in CCR erratic.","Cargo Mach.,Hull & Tanks","Cargo / Ballast Systems","Equipment Related","8.8","Medium","","","Frequent line blowing through carried out. ","2024-06-15T08:00:00","","In progress",null,"No","No","No","Internal"]
[null,null,null,null,70511,"27_Thu Mar 14 2024 23:55:32 GMT+0800","2024-03-01T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Soot tank eductor housing is found to be leaking.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Soot tank eductor is having multiple holes, new eductor is supplied but it is not operational, the size of the nozzle is big compared to the existing. Big nozzle will require more pressure to  create the venturi effect as compared with the diffuser. ","2024-05-30T08:00:00","","In progress",null,"No","No","No","Internal"]
[null,null,null,null,13594,"27_Fri Mar 15 2024 16:42:09 GMT+0800","2024-03-01T08:00:00","Defect","Ship Staff","Ship Staff Insp.","BWTS sea water after electrolyzer to Aft peak tank flow control valve FCV 3131 PCB is defective.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","The flow control valve FCV 3131 for aft peak tank is not operational as the PCB is found to be defective, same to be replaced with new PCB. Spares received in Singapore job is planned.","2024-05-30T08:00:00","DLOT230255","In progress",null,"No","No","No","Internal"]
[null,null,null,null,35916,"27_Sun May 12 2024 23:11:41 GMT+0800","2024-05-09T08:00:00","Defect","Ship Staff","Ship Staff Insp.","High expansion foam tank -Guage glass pipe line has small hole. ","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.35","Medium","","","Leak arrested by Soft repair . Permanent repair will require emptying of tank and hot work, to be planned at suitable opportunity. ","2024-07-31T08:00:00","","Not Started",null,"No","No","No","Internal"]

{"sheet":"Completed","index":1,"n_rows":1034,"n_cols":28,"rows_kept":1034,"cut":false,"hidden":false,"merged":[[10,8,10,9],[10,12,10,13],[12,6,12,27],[8,6,8,27]]}
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,"Defect - Damage Monitoring Sheet"]
[]
[null,null,null,null,null,null,null,"Date of Report","13-May-2024",null,null,"Ship Name","DHT LOTUS (04-03-2024)"]
[]
[null,null,null,null,null,null,"VERSION : 2.0"]
[]
[]
[]
[null,null,null,"ID","SHIPSIDE UNIQUEID","UNIQUE ID","Date Recorded","Type of Deficiency","Observer code","Type of Inspection","Description of Deficiency","Equipment Categories","Area of Observation","Deficiency Cause","VIQ Ref Number","Risk Value of Obs","PSC Ref Number","PSC MOU ID","Action Taken or Required","Target Date","PO Ref No.","Status Code","Date Completed","Drydock","Info Sharing","Critical Item","Audit Type","Superintendent Remarks"]
[null,null,null,2555,null,"27_15/10/2019 14:30:50","2018-12-29T23:59:35","Defect","Ship Staff","Ship Staff Insp.","GALLEY COOKING RANGE INSULATION FAULT ","Accommodation","General Appearance","Equipment Related","5.25","Medium","","","HOT PLATE REPLACED WITH A SPARE ONE- OPERATING SATISFACTORY.","2019-12-26T23:59:35","","Completed","2019-11-07T23:59:35","No","No","No","Internal"]
[null,null,null,2560,null,"27_15/10/2019 14:48:02","2018-12-30T23:59:35","Defect","Ship Staff","OM Insp. (Eg. SIRE / CDI etc.)","MOORING WINCH TO BE DE RUSTED AND PAINTED ","Deck - Mooring Machinery","Cargo / Ballast Systems","Equipment Related","9.14","Medium","","","ALL MOORING WINCHES RUSTED AND PAINTED","2019-12-26T23:59:35","","Completed","2019-10-30T23:59:35","No","No","No","Internal"]
[null,null,null,2576,null,"27_15/10/2019 13:34:34","2019-01-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","LIFE BOAT DOOR HOLDER ARRANGEMENT DAMAGED ","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.27","Medium","","","REPAIRS CARRIED OUT ","2019-01-10T23:59:35","","Completed","2019-01-02T23:59:35","No","No","No","Internal"]
[null,null,null,2578,null,"27_15/10/2019 13:50:50","2019-01-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","SIGHT GLASSES OF BOTH HOSE HANDLING CRANES DAMAGED / PAINTED OVER & NOT CLEAR ","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.63","High","","","ALL SIGHT GLASSES RENEWED ","2019-01-13T23:59:35","","Completed","2019-01-08T23:59:35","No","No","No","Internal"]
[null,null,null,2577,null,"27_15/10/2019 13:47:36","2019-01-04T23:59:35","Defect","Ship Staff","Ship Staff Insp.","ONE OF THE COW LINE U CLAMP WAS MISSING ","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.34","High","","","NEW U CLAMP FITTED ","2019-02-07T23:59:35","","Completed","2019-01-04T23:59:35","No","No","No","Internal"]
[null,null,null,2547,null,"27_15/10/2019 8:18:03 AM","2019-01-06T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Air con compressor #1 oil return chamber float broken","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","Presently functioning satisfactory.","2019-02-23T23:59:35","","Completed","2019-12-19T23:59:35","No","No","No","Internal"]
[null,null,null,2579,null,"27_15/10/2019 13:55:00","2019-01-07T23:59:35","Defect","Ship Staff","Ship Staff Insp.","W2 INOARD WINCH - WIRE END SECURING PLATE ALONG WITH STUD BOLTS DAMAGED DURING TRANSFERING OF WIRE ","Deck - Mooring Machinery","Mooring","Equipment Related","9.14","Medium","","","NEW P- PLATE ALONG WITH STUD BOLTS RENEWED & FITTED TO W2 DRUM PLATE ","2019-01-08T23:59:35","","Completed","2019-01-08T23:59:35","No","No","No","Internal"]
[null,null,null,2581,null,"27_15/10/2019 14:02:06","2019-01-07T23:59:35","Defect","Ship Staff","Ship Staff Insp.","ALL 4 VECS MANIFOLD 12 CLOCK POSITION STUD BOLTS FOUND WASTED ","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","","","","","ALL 4 RENEWED ","2019-01-14T23:59:35","","Completed","2019-01-09T23:59:35","No","No","No","Internal"]
[null,null,null,2580,null,"27_15/10/2019 13:59:22","2019-01-08T23:59:35","Defect","Ship Staff","Ship Staff Insp.","WIRE LASHING OF SECURING PIPES NOT FOUND ON PORT FUNNEL DECK WERE FOUND PARTLY DAMAGED DUE TO CORRISION ","Deck - Machinery","General Appearance","Equipment Related","5.11","Low","","","LASHING RENEWED ","2019-01-10T23:59:35","","Completed","2019-01-08T23:59:35","No","No","No","Internal"]
[null,null,null,2582,null,"27_15/10/2019 14:05:06","2019-01-09T23:59:35","Defect","Ship Staff","Ship Staff Insp.","1 FOAM LINE & FIRE LINE DRESSOR COUPLING FOUND LEAKING ","LSA / FFA","Safety / LSA / FFA","External Factors","","","","","WEDGE RINGS RENEWED .LEAK ARRESTED ","2019-01-15T23:59:35","","Completed","2019-01-10T23:59:35","No","No","No","Internal"]
[null,null,null,2556,null,"27_15/10/2019 14:34:16","2019-01-09T23:59:35","Defect,Other","Ship Staff","Ship Staff Insp.","NIGHT VISION BINOCULARS NON FUNCTIONAL ","Navigation - Others","Navigation","Equipment Related","7.4","Low","","","NEW  BINOCULARS RECEIVED","2019-12-26T23:59:35","","Completed","2019-03-30T23:59:35","No","No","No","Internal"]
[null,null,null,2583,null,"27_15/10/2019 14:18:47","2019-01-11T23:59:35","Defect","Ship Staff","Ship Staff Insp.","OFFICER MESS ROOM VENT FLAP RETAINING CHANNEL FOUND DAMAGED ","Accommodation ,Deck - Machinery","General Appearance","Equipment Related","11.13","Low","","","SAME FABRICATED AND RUBBER PACKING RENEWED ","2019-01-14T23:59:35","","Completed","2019-01-12T23:59:35","No","No","No","Internal"]
[null,null,null,2561,null,"27_15/10/2019 8:23:15 AM","2019-01-15T23:59:35","Defect","Ship Staff","Ship Staff Insp.","LP circulating pump #1 not operational","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","pump opened up found bearing bush damaged need overhaul spares ordered","2019-02-05T23:59:35","DLOT190071","Completed","2019-08-01T23:59:35","No","No","No","Internal"]
[null,null,null,2557,null,"27_15/10/2019 14:38:57","2019-01-30T23:59:35","Defect","Ship Staff","Ship Staff Insp.","DECK SEAL OVERBOARD LINE INBOARD VALVE LEAKING FROM FLANGE IN PUMPROOM PORT SIDE ","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.27","Medium","","","VALVE REPLACED-NO LEAKS OBSERVED. ","2019-12-26T23:59:35","","Completed","2019-08-31T23:59:35","No","No","No","Internal"]
[null,null,null,2558,null,"27_15/10/2019 14:40:44","2019-01-30T23:59:35","Defect","Ship Staff","Ship Staff Insp.","CARGO VALVE CAV 188 ACTUATOR LEAKING ","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.44","High","","","ACTUATOR REPLACED-NO LEAKS OBSERVED","2019-12-25T23:59:35","","Completed","2019-08-31T23:59:35","No","No","No","Internal"]
[null,null,null,2559,null,"27_15/10/2019 14:44:29","2019-01-30T23:59:35","Defect","Ship Staff","Ship Staff Insp.","PLATFORM FOR CHANGING LIGHT IN PUMP ROOM UPPR PLATFORM NOT FITTED WITH GUARD RAILS ","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","GUARD RAILS FITTED IN YULIAN SHIPYARD.","2019-12-26T23:59:35","","Completed","2019-09-04T23:59:35","No","No","No","Internal"]
[null,null,null,2562,null,"27_15/10/2019 8:29:51 AM","2019-02-15T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Exhaust leakage observed from by-pass damper shaft bearings","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","valve to inspect and bearing to renew","2019-05-26T23:59:35","","Completed","2019-08-03T23:59:35","No","No","No","Internal"]
[null,null,null,2563,null,"27_15/10/2019 8:39:09 AM","2019-02-15T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ME LO auto backwash filter not turning","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.7","Medium","","","Spares received. Filters opened up and cleaned hydraulic unit motors and spares renewed","2019-04-25T23:59:35","DLOT190079","Completed","2019-08-09T23:59:35","No","No","No","Internal"]
[null,null,null,2550,null,"27_15/10/2019 8:35:57 AM","2019-02-15T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Oil leakage observed from Aft of local manoeuvring platform, source to be identified\t","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Oil leaks rectified.","2019-07-26T23:59:35","","Completed","2019-11-13T23:59:35","No","No","No","Internal"]
[null,null,null,2564,null,"27_15/10/2019 8:41:52 AM","2019-03-13T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Aft LT cooler sea water inlet pipe holed.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Temporary repair carried out with Devcon, pipe to be removed and renewed or welded repair carried out.\n\nDD spec raised for same in REFMAN.\n\n","2019-04-25T23:59:35","","Completed","2019-08-21T23:59:35","Yes","No","No","Internal"]
[null,null,null,2584,null,"27_15/10/2019 14:53:20","2019-03-16T23:59:35","Defect","Ship Staff","Ship Staff Insp.","MOORING WINCH M1 / M4 / M5 HYDRAULIC LEAK ","E/R - Boiler,Deck - Mooring Machinery","Mooring","Equipment Related","9.14","Medium","","","M4 AND M5 NEW BLOCK WITH ORINGS AND SHAFT RENEWED LEAKAGES RECTIFIED M1 HAS NO LEAKS ","2019-04-25T23:59:35","","Completed","2019-04-07T23:59:35","No","No","No","External"]
[null,null,null,2586,null,"27_15/10/2019 14:59:15","2019-03-25T23:59:35","Defect","Ship Staff","Ship Staff Insp.","NEW SLINGS , CHAIN BLOCKS AS PER SAFETY FLASH 81 TO BE PROCURED ","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.11","Low","","","REQN RAISED / AWAITING SPARES ","2019-04-25T23:59:35","","Completed","2019-04-22T23:59:35","No","No","No","External"]
[null,null,null,2585,null,"27_15/10/2019 14:56:38","2019-04-15T23:59:35","Defect","Ship Staff","Ship Staff Insp.","FIRE AND GS PUMP MECHNICAL SEAL LEAKING ","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.35","Medium","","","MECHNIACL SEAL RENEWED AT SUITABLE OPPORTUNITY ","2019-05-11T23:59:35","","Completed","2019-07-22T23:59:35","No","No","No","Internal"]
[null,null,null,2565,null,"27_15/10/2019 9:11:01 AM","2019-04-22T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","#1 & #3 Main Feed water pumps disch gauges needle found broken. ","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.31","Very High","","","vessel needs to order the pressure gauge 0- 40 bar in next store.","2019-07-22T23:59:35","","Completed","2019-09-17T23:59:35","No","No","No","Internal"]
[null,null,null,2551,null,"27_15/10/2019 9:01:27 AM","2019-04-22T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Aft Hydraulic storage tank gauge glass leaking","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","Leakage rectified by renewing the o-rings.","2019-07-25T23:59:35","","Completed","2019-11-22T23:59:35","No","No","No","Internal"]
[null,null,null,2552,null,"27_15/10/2019 9:04:55 AM","2019-04-22T23:59:35","Defect","Ship Staff","Ship Staff Insp.","DG lube oil settling and service tanks gauge glasses leaking.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","Gauge glass leakage rectified by replacing the o-rings.","2019-07-25T23:59:35","","Completed","2019-11-21T23:59:35","No","No","No","Internal"]
[null,null,null,2566,null,"27_15/10/2019 9:14:19 AM","2019-04-27T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Deck Seal - Pnuematic vent valve to atmosphere not-operational","Inert Gas","Cargo / Ballast Systems","Equipment Related","","","","","Trobleshooting in progress. Requisition to be raised for spares.","2019-07-27T23:59:35","","Completed","2019-08-03T23:59:35","No","No","No","Internal"]
[null,null,null,2553,null,"27_15/10/2019 9:18:29 AM","2019-05-05T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Cylinder oil daily tank gauge glass leaking from bottom valve","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","Top and bottom valve o-rings renewed","2019-08-10T23:59:35","","Completed","2019-11-21T23:59:35","No","No","No","Internal"]
[null,null,null,2567,null,"27_15/10/2019 9:22:23 AM","2019-05-10T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Aft ICCP display not working","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","Troubleshooting carried out, input power available to PCB, concluded display defective, RO raised","2019-08-09T23:59:35","DLOT190111","Completed","2019-09-17T23:59:35","No","No","No","Internal"]
[null,null,null,2554,null,"27_15/10/2019 9:25:20 AM","2019-05-27T23:59:35","Defect","Ship Staff","Ship Staff Insp.","44OV low Insulation  from ICO Lube power panel,Micromaster siemens.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","As per the e-mail from lukoil ,V/L to keep Icolub swiched off when not in operation,otherwise,to buy a transformer from them to put in E/E.","2019-08-27T23:59:35","","Completed","2019-12-07T23:59:35","No","No","No","Internal"]
[null,null,null,2568,null,"27_15/10/2019 9:30:45 AM","2019-06-02T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Fog local fire fighting system Battery Fault.","Elect. Mach. & Equip.","Safety / LSA / FFA","Equipment Related","","","","","Full system renewed","2019-09-02T23:59:35","","Completed","2019-09-05T23:59:35","No","No","No","Internal"]
[null,null,null,2569,null,"27_15/10/2019 10:15:11 AM","2019-06-10T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Low sea chest suction valve remote operation hydralic leakage","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.31","Very High","","","During isolation for sea suction strainer cleaning the valve operated from remote hydralic system, found heavy oil leakage in the valve spindle , due to that valve is not closing fully.Vessel dont have manual for this particular valve to order any seals. Presently local manual operating hand wheel engaged and can operate manually from local position. valve need to be overhaul during drydock","2019-09-10T23:59:35","","Completed","2019-08-20T23:59:35","Yes","No","No","Internal"]
[null,null,null,2570,null,"27_15/10/2019 10:17:53 AM","2019-06-14T23:59:35","Defect","Ship Staff","Ship Staff Insp.","AE no.2 air cooler holding bolts seized in place","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Vessel planned for aircooler cleaning for no.2 aux engine. During opening found all the bolts are very hard to open, somehow managed to open the bolts except 2 pieces, which is seized in place. 2 bolts which is located inside the air intlet piece also found seized. various attempts made to open the seized bolts but couldn't succeed","2019-09-14T23:59:35","","Completed","2019-08-27T23:59:35","Yes","No","No","Internal"]
[null,null,null,2571,null,"27_15/10/2019 10:19:22 AM","2019-06-26T23:59:35","Defect","Ship Staff","Ship Staff Insp.","No.1HFO service tank heating coil outlet steam trap leaking","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Steam trap has to be overhauled","2019-09-26T23:59:35","","Completed","2019-08-11T23:59:35","No","No","No","Internal"]
[null,null,null,2572,null,"27_15/10/2019 10:21:39 AM","2019-06-27T23:59:35","Defect","Ship Staff","Ship Staff Insp.","FWD LT cooler S.W outlet pipe reducer leaking","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Temporary repairs carried out, leak arrested, need to renew the pipe at suitable opportunity","2019-09-27T23:59:35","","Completed","2019-08-21T23:59:35","No","No","No","Internal"]
[null,null,null,2573,null,"27_15/10/2019 10:23:52 AM","2019-06-27T23:59:35","Defect","Ship Staff","Ship Staff Insp.","COPT vaccum condenser bypass valve body get holed and leaking","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","8.33","Medium","","","Temporary repair carried out, leakage minimised, need to renew the valve","2019-09-27T23:59:35","","Completed","2019-08-11T23:59:35","No","No","No","Internal"]
[null,null,null,2574,null,"27_15/10/2019 10:27:26 AM","2019-06-28T23:59:35","Defect","Ship Staff","Ship Staff Insp.","COPT vaccum condensor S.W inlet pipe leaking","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","8.33","Medium","","","Temporary repair carried out, pipe section needs to be renewed","2019-09-28T23:59:35","","Completed","2019-08-11T23:59:35","No","No","No","Internal"]
[null,null,null,2575,null,"27_15/10/2019 10:29:43 AM","2019-06-28T23:59:35","Defect","Ship Staff","Ship Staff Insp.","All 3 COPT LO cooler oil side leaking","Cargo Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Cooler has to be inspected and packing need to be renewed during docking","2019-09-28T23:59:35","","Completed","2019-08-28T23:59:35","No","No","No","Internal"]
[null,null,null,5707,null,"27_43779.653599537","2019-09-08T23:59:35","Critical Equipment","Ship Staff","Ship Staff Insp.","Fire alarm showing fault ","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.35","Medium","","","smoke sensor and manual call point needed for attendence.Manual call point renewed and system is functioning satisfactory.","2019-10-25T23:59:35","DLO190178 and DLOT190210","Completed","2019-10-23T23:59:35","No","No","No","Internal"]
[null,null,null,9149,null,"27_43779.6572569444","2019-09-08T23:59:35","Other","Ship Staff","Ship Staff Insp.","Diffusers for light fittings in engine room  damaged/cracked/broken at various locations post dd ","Critical Equip.,Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.25","Very High","","","Diffusers replaced as required.","2019-10-25T23:59:35","","Completed","2019-12-01T23:59:35","No","No","No","Internal"]
[null,null,null,9150,null,"27_Sun Nov 10 2019 15:49:57 GMT+0000 (Coordinated Universal Time)","2019-09-08T23:59:35","Other","Ship Staff","Ship Staff Insp.","Engine room alarm column light and sound non functional in various locations post dd","Cargo Mach.,Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.15","Low","","","E/R alarm columns made operational ","2019-10-25T23:59:35","DLOT190205","Completed","2019-12-02T23:59:35","No","No","No","Internal"]
[null,null,null,2536,null,"27_2019-11-10 15:41:11.000","2019-09-08T23:59:35","Critical Equipment","Ship Staff","Ship Staff Insp.","Fire alarm showing fault ","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.35","Medium","","","Smoke sensor and manual call point needed for attendence. \n\nSmoke sensor and manual call point sensor renewed and found satisfactory.","2019-10-25T23:59:35","dlot190178 and dlot190210","Completed","2019-10-23T23:59:35","No","No","No","Internal"]
[null,null,null,2537,null,"27_2019-11-10 15:46:27.000","2019-09-08T23:59:35","Other","Ship Staff","Ship Staff Insp.","Diffusers for light fittings in engine room  damaged/cracked/broken at various locations post dd ","Critical Equip.,Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.25","Very High","","","Diffusers replaced as required","2019-10-25T23:59:35","","Completed","2019-12-01T23:59:35","No","No","No","Internal"]
[null,null,null,2538,null,"27_2019-11-10 15:49:57.999","2019-09-08T23:59:35","Other","Ship Staff","Ship Staff Insp.","Engine room alarm column light and sound non functional in various locations post dd","Cargo Mach.,Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.15","Low","","","Engine room alarm columns made operational ","2019-10-25T23:59:35","dlot190205","Completed","2019-12-02T23:59:35","No","No","No","Internal"]
[null,null,null,9129,null,"27_Sun Nov 10 2019 15:53:50 GMT+0000 (Coordinated Universal Time)","2019-09-13T23:59:35","Other","Ship Staff","Ship Staff Insp.","A/E no 3 crank case getting pressurized ","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","crankcase vent line newly fabricated to nominal dia 80A as per makers reccomendation","2019-12-26T23:59:35","dlot 190216","Completed","2019-11-12T23:59:35","No","No","No","Internal"]
[null,null,null,2539,null,"27_2019-11-10 15:53:50.000","2019-09-13T23:59:35","Other","Ship Staff","Ship Staff Insp.","A/E no 3 crank case getting pressurized ","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","A/E no.3 crankcase vent line newly fabricated to nominal dia 80A as per maker's recommendation","2019-12-26T23:59:35","dlot 190216","Completed","2019-11-12T23:59:35","No","No","No","Internal"]
[null,null,null,9132,null,"27_Sun Nov 10 2019 15:58:11 GMT+0000 (Coordinated Universal Time)","2019-09-15T23:59:35","Other","Ship Staff","Ship Staff Insp.","LSMGO Main line manifold valve is not with gear operated ","Deck - Pipe / Fittings","Eng. / Strg. Comp.","Equipment Related","6.7","High","","","LSMGO main maniflod fitted with gear operated valves","2019-12-25T23:59:35","","Completed","2019-11-20T23:59:35","No","No","No","Internal"]
[null,null,null,2540,null,"27_2019-11-10 15:58:11.999","2019-09-15T23:59:35","Other","Ship Staff","Ship Staff Insp.","LSMGO Main line manifold valve is not with gear operated ","Deck - Pipe / Fittings","Eng. / Strg. Comp.","Equipment Related","6.7","High","","","LSMGO main line manifold fitted with gear operated valves","2019-12-25T23:59:35","dlot 190216","Completed","2019-11-20T23:59:35","No","No","No","Internal"]
[null,null,null,9081,null,"27_43779.6758912037","2019-09-21T23:59:35","Other","Ship Staff","Ship Staff Insp.","Pumproom gas detection system sensor non functional ","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.21","High","","","Pumproom Bottom Stbd HC Sensor Renewed","2019-11-25T23:59:35","dlot 190008","Completed","2019-11-09T23:59:35","No","No","No","Internal"]
[null,null,null,2541,null,"27_2019-11-10 16:13:17.000","2019-09-21T23:59:35","Other","Ship Staff","Ship Staff Insp.","Pumproom gas detection system sensor non functional ","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.21","High","","","Pumproom Bottom STBD HC sensor renewed","2019-11-25T23:59:35","dlot 190008","Completed","2019-11-09T23:59:35","No","No","No","Internal"]
[null,null,null,5703,null,"27_2019-11-10 16:15:18.999","2019-09-27T23:59:35","Other","Ship Staff","Ship Staff Insp.","Anemometer in CCR is non functional ","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","5.9","Very High","","","Restored windows in the system - functioning satiisfactory","2019-10-25T23:59:35","","Completed","2019-10-31T23:59:35","No","No","No","Internal"]
[null,null,null,9076,null,"27_43779.6773032407","2019-09-27T23:59:35","Other","Ship Staff","Ship Staff Insp.","Anemometer in CCR is non functional ","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","5.9","Very High","","","RESTORED THE WINDOWS IN THE SYSTEM-FUNCTIONING SATISFACTORY.","2019-10-25T23:59:35","","Completed","2019-10-31T23:59:35","No","No","No","Internal"]
[null,null,null,9178,null,"27_Sun Nov 10 2019 16:17:26 GMT+0000 (Coordinated Universal Time)","2019-09-27T23:59:35","Other","Ship Staff","Ship Staff Insp.","No 1 Stbd Cargo tank temperature sensor is non functional ","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.37","High","","","Techincian attended the V/L at Singapore on 18th Nov.2019 and suggested to renew the junction box which V/L will install as the time permits.","2019-11-25T23:59:35","","Completed","2019-12-21T23:59:35","No","No","No","Internal"]
[null,null,null,2542,null,"27_2019-11-10 16:15:19.000","2019-09-27T23:59:35","Other","Ship Staff","Ship Staff Insp.","Anemometer in CCR is non functional ","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","5.9","Very High","","","Restored the windows in the system  - functioning satisfactorily","2019-10-25T23:59:35","","Completed","2019-10-31T23:59:35","No","No","No","Internal"]
[null,null,null,2543,null,"27_2019-11-10 16:17:26.999","2019-09-27T23:59:35","Other","Ship Staff","Ship Staff Insp.","No 1 Stbd Cargo tank temperature sensor is non functional ","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.37","High","","","Technician attendance the V/L at Singapore on 18NOV2019 and suggested to renew the junction box which vessel will install as the time permits","2019-11-25T23:59:35","","Completed","2019-12-21T23:59:35","No","No","No","Internal"]
[null,null,null,2544,null,"27_2019-11-10 16:20:15.000","2019-09-29T23:59:35","Defect","Ship Staff","Ship Staff Insp.","A/E no 3 smoke and heat detector is getting activated in heat mode while DG is in operation ","E/R - Aux. Mach.,LSA / FFA","Eng. / Strg. Comp.","Equipment Related","5.35","Medium","","","Detectors to be repositioned to higher areas ","2019-11-25T23:59:35","","Completed","2019-10-12T23:59:35","No","No","No","Internal"]
[null,null,null,9107,null,"27_16/11/2019 07:49:53","2019-10-01T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Earthing Wire for the flow meter for Scrubber line to be secured","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Behaviour Based,Human Error","","","","","Earthing Wire checked & Secured properly","2019-11-25T23:59:35","","Completed","2019-11-11T23:59:35","No","No","No","Internal"]
[null,null,null,9077,null,"27_Sun Nov 10 2019 16:25:11 GMT+0000 (Coordinated Universal Time)","2019-10-05T23:59:35","Other","Ship Staff","Ship Staff Insp.","Stbd Windlass brake assembly leaky due to scoring of rams ","Deck - Machinery,Deck - Mooring Machinery","Mooring","Equipment Related","9.14","Medium","","","SHAFT BUILD UP BELZONA AND SMOOTHENED.SEALS REPACED.","2019-10-25T23:59:35","","Completed","2019-10-27T23:59:35","No","No","No","Internal"]
[null,null,null,9184,null,"27_Sun Nov 10 2019 16:22:13 GMT+0000 (Coordinated Universal Time)","2019-10-05T23:59:35","Other","Ship Staff","Ship Staff Insp.","Draft gauges are non functional ","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.2","Medium","","","Technician expects to attend V/L at Zhoushan  about 28th Dec.2019","2019-11-25T23:59:35","DLOT 190219 ","Completed","2019-12-21T23:59:35","No","No","No","Internal"]
[null,null,null,2545,null,"27_2019-11-10 16:22:13.999","2019-10-05T23:59:35","Other","Ship Staff","Ship Staff Insp.","Draft gauges are non functional ","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.2","Medium","","","Technician expects to attend vessel at Zhoushan about 28DEC2019","2019-11-25T23:59:35","DLOT 190219 ","Completed","2019-12-21T23:59:35","No","No","No","Internal"]
[null,null,null,2546,null,"27_2019-11-10 16:25:11.999","2019-10-05T23:59:35","Other","Ship Staff","Ship Staff Insp.","Stbd Windlass brake assembly leaky due to scoring of rams ","Deck - Machinery,Deck - Mooring Machinery","Mooring","Equipment Related","9.14","Medium","","","Shaft build up Belzona and smoothened. Seals replaced.","2019-10-25T23:59:35","","Completed","2019-10-27T23:59:35","No","No","No","Internal"]
[null,null,null,5704,null,"27_21/10/2019 4:11:35 PM","2019-10-11T23:59:35","Defect","Ship Staff","Ship Staff Insp.","FAILURE OF AC-DC CONVERTER UNIT FOR  M/E RPLS","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","PSU UNIT REPLACED AND SYSTEM FOUND TO BE WORKING STAISFACTORY","2019-12-11T23:59:35","RO DLOT 190227 RAISED","Completed","2019-10-30T23:59:35","No","No","No","Internal"]
[null,null,null,5701,null,"27_21/10/2019 4:24:18 PM","2019-10-16T23:59:35","Defect","Ship Staff","Ship Staff Insp.","EMG.GENERATOR ROOM STBD.SIDE VENT FLAP SEIZED","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","FlLAP VANES OBSERVED TO BE BADLY RUSTED,NEEDS TO BE CHIPPED AND PAINTED.ALL DONE-OPERATING SATIS.","2019-10-25T23:59:35","","Completed","2019-10-23T23:59:35","No","No","No","Internal"]
[null,null,null,5705,null,"27_29/10/2019 1:26:36 PM","2019-10-21T23:59:35","Guarantee Claim","Ship Staff","Ship Staff Insp.","SOX SCRUBBER FLOW METER DEFECTIVE","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","GUARANTEE SERVICE ENGR. ATTENDED THE V/L AT ULSAN AND REPLACED THE PCB BOARD INSIDE THE FLOWMETER CARTRIDGE-OPERATION SATISFACTORY","2019-12-20T23:59:35","","Completed","2019-11-01T23:59:35","No","No","No","Internal"]
[null,null,null,5700,null,"27_29/10/2019 5:18:47 PM","2019-10-22T23:59:35","Defect","Ship Staff","Ship Staff Insp.","VENT FLAPS AT ECONOMISER LP PLATFORM & SCRUBBER ROOM TURNING VERY HARD","Miscellaneous","Emgcy. Systems","Equipment Related","","","","","VENT FLAPS REMOVED FROM PLACE,EASED UP IN THE W/SHOP AND BOXED BACK-SATISFACTORY","2019-10-25T23:59:35","","Completed","2019-10-22T23:59:35","No","No","No","Internal"]
[null,null,null,5706,null,"27_29/10/2019 5:31:35 PM","2019-10-23T23:59:35","Other","Ship Staff","Ship Staff Insp.","Erratic  PLC Controller of refrigeration control panel.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","Observed for more than a month and no problem experienced.","2019-12-20T23:59:35","","Completed","2019-12-02T23:59:35","No","No","No","Internal"]
[null,null,null,5702,null,"27_29/10/2019 5:36:28 PM","2019-10-24T23:59:35","Defect","Ship Staff","Ship Staff Insp.","NO1 & NO.2 HFO SETT TANK O'FLOW PIPE GAUGE GLASS LEAKING","Deck - Pipe / Fittings","Eng. / Strg. Comp.","Equipment Related","","","","","GAUGE GLASS RENEWED WITH A SPARE ONE","2019-10-26T23:59:35","","Completed","2019-10-24T23:59:35","No","No","No","Internal"]
[null,null,null,9071,null,"27_Sun Aug 11 2019 11:06:24 GMT+0000 (Coordinated Universal Time)","2019-10-27T23:59:35","Defect","Ship Staff","Ship Staff Insp.","B/R MIDDLE WINDOW WIPER INOPERATIONAL.","Elect. Mach. & Equip.","Navigation","Equipment Related","","","","","COMLETE WIPER ASSY REMOVED FROM PLACE ,AND INSPECTED.OBERVED BELT GUIDE LOCKING BOLTS WORN OUT,SAME REPLACED AND WIPER FOUND TO OPERATING SATISFAC TORY.","2019-10-30T23:59:35","","Completed","2019-10-27T23:59:35","No","No","No","Internal"]
[null,null,null,9082,null,"27_Fri Nov 08 2019 11:13:31 GMT+0000 (Coordinated Universal Time)","2019-10-27T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","PUMP RM HC SENSOR STBD SIDE NOT GIVING ANY OUTPUT DURING CALIBRATION","Elect. Mach. & Equip.","Cargo / Ballast Systems","Equipment Related","","","","","HC  SENSOR Pumproom Bottom Stbd Replaced.Zero & Span Gas Calibration Done","2019-11-03T23:59:35","","Completed","2019-11-09T23:59:35","No","No","No","Internal"]
[null,null,null,9182,null,"27_16/11/2019 8:36:16 AM","2019-10-27T23:59:35","Critical Equipment","Ship Staff","Ship Staff Insp.","Bridge UPS was not operational\t\t","Navigation - Others","Navigation","Equipment Related","","","",""," NO 1 UPS RENEWED BY SHORE TECHNICIAN AT SINGAPORE ON 18TH DEC 2019 AND ALL FOUND TO BE IN ORDE4R. OBSERVATION","2019-11-25T23:59:35","","Completed","2019-12-21T23:59:35","No","No","No","Internal"]
[null,null,null,2549,null,"27_15/10/2019 8:33:47 AM","2019-10-28T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","DG # 1 oilmax pump leaking","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Seal renewed","2020-01-25T23:59:35","DLOT190074","Completed","2020-01-15T23:59:35","No","No","No","Internal","Spares arranged at Singapore 25th Jan - earlier spares arranged where of wrong supply."]
[null,null,null,9072,null,"27_Fri Oct 11 2019 19:54:37 GMT+0000 (Coordinated Universal Time)","2019-10-30T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","VECS sensor was damaged","Deck - Machinery","Cargo / Ballast Systems","Equipment Related","","","","","New sensor recevied and renewed ","2020-11-15T23:59:35","","Completed","2019-11-06T23:59:35","No","No","No","Internal"]
[null,null,null,9055,null,"27_16/11/2019 07:04:51","2019-11-01T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Strong Draft of air coming from side of AC Duct & Black stain was visible","Miscellaneous","Eng. / Strg. Comp.","Behaviour Based,Human Error","","","","","Black stain marks cleared.","2019-11-25T23:59:35","","Completed","2019-11-12T23:59:35","No","No","No","Internal"]
[null,null,null,9056,null,"27_Mon Nov 11 2019 18:39:37 GMT+0000 (Coordinated Universal Time)","2019-11-01T23:59:35","Other","Ship Staff","Ship Staff Insp.","Aux blr.no.1 flaming out intermittently.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Flame scanner renewed and boiler is operating satisfactory.","2020-01-26T23:59:35","DLOT190240 APPLIES","Completed","2020-02-28T23:59:35","No","No","No","Internal","Spares arranged delivery at Singapore 25th Jan"]
[null,null,null,9057,null,"27_15/11/2019 11:03:07 AM","2019-11-01T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","1S COT Temperature Sensor showing no readout","Miscellaneous","Cargo / Ballast Systems","Equipment Related","8.13","Medium","","","Sensor checked-Ok.Junction box replaced and it shows the proper temp.","2020-01-26T23:59:35","","Completed","2020-01-23T23:59:35","No","No","No","Internal"]
[null,null,null,9058,null,"27_15/11/2019 11:04:43 AM","2019-11-01T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","No.1 & No.3 COP Vibration Sensor Showing Erratic Readings while stopped","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.8","Medium","","","Presently no problem experienced.V/L has spare sensors and will replace as required.","2020-01-26T23:59:35","DLOT 190230","Completed","2020-01-24T23:59:35","No","No","No","Internal","Spares arranged at Singapore 25th Jan."]
[null,null,null,9059,null,"27_15/11/2019 2:16:56 PM","2019-11-01T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Fireman radios were located on the bridge. Suggest they may be relocated near fireman's locker.","LSA / FFA","Safety / LSA / FFA","Knowledge Based","","","","","Relocation done","2019-11-25T23:59:35","","Completed","2019-12-10T23:59:35","No","No","No","Internal"]
[null,null,null,9060,null,"27_15/11/2019 2:19:04 PM","2019-11-01T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","PORT & STBD lifeboats' hook does not have indication/marking for open/shut","LSA / FFA","Safety / LSA / FFA","Inappropriate Procedure","5.28","Very High","","","Open shut marking done in both life boat hook assembly","2020-01-20T23:59:35","","Completed","2020-01-19T23:59:35","No","No","No","Internal"]
[null,null,null,9061,null,"27_15/11/2019 4:37:08 PM","2019-11-01T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ME - RPM indicator at local manoeuvring platform has an error of 10 rpm. When M/E was in STOP condition it is showing 10 RPM AHEAD.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","ME RPM indicator renewed and shows the correct RPM.","2020-06-25T23:59:35","","Completed","2020-06-13T23:59:35","No","No","No","Internal"]
[null,null,null,9062,null,"27_16/11/2019 06:24:10","2019-11-01T23:59:35","Critical Equipment,Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Draft Gauge in CCR not Working","Miscellaneous","Cargo / Ballast Systems","Equipment Related","8.23","Medium","","","Service technician attended the V/L at Singapore on 16th June 20 and found to be working satisfactory.","2020-09-08T23:59:35","","Completed","2020-06-11T23:59:35","No","No","No","Internal","Spares arranged at Singapore 25th Jan"]
[null,null,null,9063,null,"27_16/11/2019 06:25:31","2019-11-01T23:59:35","Critical Equipment,Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Stripper Pump Stroke Counter showing Erratic Readings","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.8","Medium","","","New Stroke counter installed and the old one replaced and tested. Strokes showing on the counter.","2021-02-23T23:59:35","DLOT200183 Received","Completed","2021-02-11T23:59:35","No","No","No","Internal"]
[null,null,null,9064,null,"27_16/11/2019 06:28:10","2019-11-01T23:59:35","Critical Equipment,Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","WBT Gas Detection System flow Sensor Fault","Critical Equip.","Cargo / Ballast Systems","Equipment Related","8.41","Medium","","","Troubleshooting carried out.New Sensor Installed.Technician attended the v/l on 21st Jan 2020 at Singapore and repalced the diaphragm of the sampling pump","2020-01-26T23:59:35","","Completed","2020-01-16T23:59:35","No","No","No","Internal","Technician arranged at Singapore 25th Jan"]
[null,null,null,9065,null,"27_16/11/2019 06:30:01","2019-11-01T23:59:35","Critical Equipment,Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","2nd Hydraulic Pump does not cut in on pressure drop in the system","Critical Equip.","Cargo / Ballast Systems","Equipment Related","8.18","High","","","Pressure switch needs renewal.Same defect is duplicate,hence,closed out.","2020-01-26T23:59:35","RO RAISED","Completed","2020-01-26T23:59:35","No","No","No","Internal"]
[null,null,null,9066,null,"27_16/11/2019 06:31:43","2019-11-01T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","SAAB Buzzer in CCR not audible","Miscellaneous","Cargo / Ballast Systems","Equipment Related","","","","","Will modify the ckt","2019-11-25T23:59:35","","Completed","2020-01-01T23:59:35","No","No","No","Internal"]
[null,null,null,9067,null,"27_16/11/2019 07:13:27","2019-11-01T23:59:35","Critical Equipment,Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Phones in Accomodation had missing buttons on the dialing panel","Critical Equip.,Navigation - GMDSS & Communication","Communication","Behaviour Based,Human Error","10.39","High","","","3no.phones received at Singapore on 16th June2020 and replaced the defective ones.","2020-09-01T23:59:35","DLOT200068 raised,Spares recd. at Singapore on 16th June20.","Completed","2020-06-15T23:59:35","No","No","No","Internal","Pls raise RO"]
[null,null,null,9068,null,"27_16/11/2019 10:07:33 AM","2019-11-01T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Fire line pressure in CCR doesn't show the correct reading. Always showing 2 bar.","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","Renewed pressure transmitter.Gauge in the CCR shows correct read out.","2019-11-25T23:59:35","","Completed","2020-01-01T23:59:35","No","No","No","Internal"]
[null,null,null,9069,null,"27_16/11/2019 10:22:10 AM","2019-11-01T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","SAAB alarm in the CCR is not audible. The volume intensity to be increased.","Elect. Mach. & Equip.","Cargo / Ballast Systems","Equipment Related","","","","","Buzzer installed by shore technician to increase alarm intensity","2020-01-26T23:59:35","","Completed","2020-01-07T23:59:35","No","No","No","Internal"]
[null,null,null,9073,null,"27_Fri Oct 11 2019 19:59:28 GMT+0000 (Coordinated Universal Time)","2019-11-01T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","Flow sensor was not giving any output signal in ballast tank gas detection system","Hull & Tanks","Cargo / Ballast Systems","Equipment Related","","","","","Flow sensor, PCB board and Transformer was renwed with the spare","2019-11-15T23:59:35","","Completed","2019-11-05T23:59:35","No","No","No","Internal"]
[null,null,null,9080,null,"27_15/11/2019 05:19:50","2019-11-01T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Tiles in Ship's Laundry found Broken/Cracked/missing","Miscellaneous","General Appearance","External Factors","","","","","Old Broken/ Cracked tiles removed and area patched up with cement ","2019-11-01T23:59:35","","Completed","2019-11-01T23:59:35","No","No","No","Internal"]
[null,null,null,9083,null,"27_15/11/2019 05:28:38","2019-11-01T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Stbd Provision Crane Platform Door/Safety Barrier Wasted","Miscellaneous","General Appearance","Equipment Related","","","","","New Door/Safety Barrier Fabricated","2019-11-09T23:59:35","","Completed","2019-11-09T23:59:35","No","No","No","Internal"]
[null,null,null,9084,null,"27_15/11/2019 05:31:56","2019-11-01T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Stbd Manifolad Drip Tray Ladder Steps Wasted","Miscellaneous","Structural Condn. / WT integrity ","Equipment Related","","","","","2 New Steps Fabricated","2019-11-07T23:59:35","","Completed","2019-11-07T23:59:35","No","No","No","Internal"]
[null,null,null,9085,null,"27_15/11/2019 06:09:47","2019-11-01T23:59:35","Critical Equipment,Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Slop P Temperature Repeater on CCR Panel showing Error","Miscellaneous","Cargo / Ballast Systems","Equipment Related","","","","","Repeater Panel Connection Checked & Error Rectified","2019-11-05T23:59:35","","Completed","2019-11-05T23:59:35","No","No","No","Internal"]
[null,null,null,9086,null,"27_15/11/2019 11:14:21 AM","2019-11-01T23:59:35","Critical Equipment,Defect","Owner / Marine / Tech. Suptd.,SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","Minor leak in Hydraulic room from stack of hydraulic Lines","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","Hydraulic Pump Kept Running for 3 days .No evident leak observed.No appreciable change in Hydraulic Level.All Armato Couplings tightened.Hydraulic Lines under continuos monitoring.All Valves in Hydraulic Room operated one by one.","2019-11-10T23:59:35","","Completed","2019-11-09T23:59:35","No","No","No","Internal"]
[null,null,null,9087,null,"27_15/11/2019 11:22:18 AM","2019-11-01T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Cabin Washroom Floor & Curtain were found dirty & Sanitary fittings Leaking","Accommodation","MLC Related","Behaviour Based","","","","","Washroom Flooring Cleaned.Shower Curtains Renewed.Shower Fittings Renewed","2019-11-10T23:59:35","","Completed","2019-11-09T23:59:35","No","No","No","Internal"]
[null,null,null,9088,null,"27_15/11/2019 1:47:51 PM","2019-11-01T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","SMB starter panel located in fwd store has been decommissioned.","Deck - Machinery","General Appearance","Equipment Related","","","","","Marked.","2019-11-25T23:59:35","","Completed","2019-11-10T23:59:35","No","No","No","Internal"]
[null,null,null,9089,null,"27_15/11/2019 2:21:41 PM","2019-11-01T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","STBD side lifeboat - box for lifeboat winch hoisting is broken","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","Box repaired.","2019-11-25T23:59:35","","Completed","2019-11-09T23:59:35","No","No","No","Internal"]
[null,null,null,9090,null,"27_15/11/2019 4:25:47 PM","2019-11-01T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","E/R - slight leak from one of the valves for the hot water tank/circulating pump","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Flange tightened and leakage rectified","2019-11-10T23:59:35","","Completed","2019-11-07T23:59:35","No","No","No","Internal"]
[null,null,null,9091,null,"27_15/11/2019 4:51:26 PM","2019-11-01T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","CCR - VECS system has a constant alarm 31. Loop, displayed.","Elect. Mach. & Equip.","Cargo / Ballast Systems","Equipment Related","","","","","Sensor Renewed.Fault rectified","2019-11-10T23:59:35","","Completed","2019-11-05T23:59:35","No","No","No","Internal"]
[null,null,null,9092,null,"27_15/11/2019 2:45:10 PM","2019-11-01T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Indicator plate for 1S COT IG valve is fitted in opposite direction","Cargo Mach.,Deck - Pipe / Fittings,Inert Gas","Cargo / Ballast Systems","Equipment Related","","","","","1S IG Valve Gear Renewed","2019-11-25T23:59:35","","Completed","2019-11-10T23:59:35","No","No","No","Internal"]
[null,null,null,9093,null,"27_15/11/2019 3:09:18 PM","2019-11-01T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Pumproom - last inspection date for the port side void space to be marked - located on deck above pumproom bottom","Miscellaneous","Cargo / Ballast Systems","Human Error,Inappropriate Procedure","","","","","Pumproom Void Space Inspected & new Date marked","2019-11-25T23:59:35","","Completed","2019-11-10T23:59:35","No","No","No","Internal"]
[null,null,null,9094,null,"27_15/11/2019 05:24:45","2019-11-01T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Weathertight Doors Channels Found Wasted - Deck Workshop/Steering Gear","Miscellaneous","Structural Condn. / WT integrity ","Equipment Related","","","","","New Channels fabricated","2019-11-11T23:59:35","","Completed","2019-11-10T23:59:35","No","No","No","Internal"]
[null,null,null,9095,null,"27_15/11/2019 1:52:00 PM","2019-11-01T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","STBD side midship store has lot of loose U clamps lying which can easily slip during rolling","Deck - Pipe / Fittings","General Appearance","Equipment Related","","","","","U-Bolts Secured.Battons in Place","2019-11-25T23:59:35","","Completed","2019-11-05T23:59:35","No","No","No","Internal"]
[null,null,null,9096,null,"27_15/11/2019 1:54:05 PM","2019-11-01T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","STBD side aft MARPOL line manifold has 2 reducers fitted","Deck - Pipe / Fittings","MARPOL Related","Equipment Related","","","","","Reducer Removed.Line Blanked","2019-11-25T23:59:35","","Completed","2019-11-07T23:59:35","No","No","No","Internal"]
[null,null,null,9097,null,"27_15/11/2019 2:29:34 PM","2019-11-01T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","SOPEP air diaphragm pump rigged at the break of accomodation was tried out and found an air leak at the connection between the flexible pipe and flexible piping.","Deck - Pipe / Fittings","MARPOL Related","Equipment Related","","","","","Leak Rectified.Rubber Packing for hose Coupling Renewed","2019-11-25T23:59:35","","Completed","2019-11-06T23:59:35","No","No","No","Internal"]
[null,null,null,9098,null,"27_15/11/2019 2:39:08 PM","2019-11-01T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Entrance to Incinerator room has been incorrectly marked as \"Garbage room\"","Miscellaneous","General Appearance","Human Error","","","","","Label Removed","2019-11-25T23:59:35","","Completed","2019-11-06T23:59:35","No","No","No","Internal"]
[null,null,null,9099,null,"27_15/11/2019 2:07:06 PM","2019-11-01T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","5S WBT sounding pipe's threads are wasted","Deck - Pipe / Fittings,Hull & Tanks","MARPOL Related","Equipment Related","","","","","New Threads made & greased.","2019-11-25T23:59:35","","Completed","2019-11-06T23:59:35","No","No","No","Internal"]
[null,null,null,9100,null,"27_15/11/2019 4:19:22 PM","2019-11-01T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Pumproom - EEBD storage box in the pump room bottom is not secured properly in pace and lying loose on the grating.","LSA / FFA","Safety / LSA / FFA","Human Error,Inappropriate Procedure","","","","","EEBD box Removed.EEBD secured on the hooks","2019-11-25T23:59:35","","Completed","2019-11-10T23:59:35","No","No","No","Internal"]
[null,null,null,9101,null,"27_15/11/2019 2:35:13 PM","2019-11-01T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","In paint store, cargo samples are stacked on top of each other and some containers are stowed above securing bars","Miscellaneous","MARPOL Related","Human Error,Inappropriate Procedure","","","","","Cargo Samples Secured & stowed below Securing Bars","2019-11-25T23:59:35","","Completed","2019-11-05T23:59:35","No","No","No","Internal"]
[null,null,null,9102,null,"27_15/11/2019 1:39:55 PM","2019-11-01T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","IG line - Mast riser - has one sighting port located on the aft piping - the retaining ring has one bolt missing.","Deck - Pipe / Fittings,Inert Gas","MARPOL Related","Equipment Related","","","","","New bolt in place","2019-11-25T23:59:35","","Completed","2019-11-09T23:59:35","No","No","No","Internal"]
[null,null,null,9103,null,"27_16/11/2019 06:40:46","2019-11-01T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Duty messroom Bulkheads found dirty with oil stains","Accommodation","General Appearance","Behaviour Based,Human Error","","","","","Bulkheads Cleaned","2019-11-10T23:59:35","","Completed","2019-11-08T23:59:35","No","No","No","Internal"]
[null,null,null,9104,null,"27_16/11/2019 07:20:21","2019-11-01T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Engine Room Workshop deck metal plated were not properly secured","Miscellaneous","Eng. / Strg. Comp.","Behaviour Based,Human Error","","","","","Plates secured properly at designated area.","2019-11-25T23:59:35","","Completed","2019-11-10T23:59:35","No","No","No","Internal"]
[null,null,null,9105,null,"27_16/11/2019 07:43:55","2019-11-01T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Floor plate for Hot Well outside ECR found with Soft Patches","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Behaviour Based,Human Error","","","","","Floor plate chipped off completely, freshly primered and painted.","2019-11-25T23:59:35","","Completed","2019-11-10T23:59:35","No","No","No","Internal"]
[null,null,null,9106,null,"27_16/11/2019 08:29:00","2019-11-01T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","One Sling strap was found hanging on an overhead pipe located near soot collecting Tank","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Behaviour Based,Human Error","","","","","Sling strap secured/removed.","2019-11-25T23:59:35","","Completed","2019-11-10T23:59:35","No","No","No","Internal"]
[null,null,null,9108,null,"27_16/11/2019 08:13:46","2019-11-01T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Control Panel for Gen. service & Control Air Compressor is Decommisioned.Same to be marked","Miscellaneous","Eng. / Strg. Comp.","Behaviour Based,Human Error","","","","","Unit has marked as decommisioned","2019-11-25T23:59:35","","Completed","2019-11-10T23:59:35","No","No","No","Internal"]
[null,null,null,9109,null,"27_16/11/2019 8:53:13 AM","2019-11-01T23:59:35","Critical Equipment","Ship Staff","Suptd. Insp.","Securing bolts are missing for 15ppm separator thermo control box\t","Critical Equip.","Emgcy. Systems","External Factors","","","","","Bolts secured","2019-11-15T23:59:35","","Completed","2019-11-11T23:59:35","No","No","No","Internal"]
[null,null,null,9110,null,"27_15/11/2019 11:17:58 AM","2019-11-01T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Securing Bolts /Studs for Scrubber Overboard Pipe threads not protruding out of securing nut.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related,Human Error","","","","","Bolts replaced with correct size and length  ","2019-11-25T23:59:35","","Completed","2019-11-15T23:59:35","No","No","No","Internal"]
[null,null,null,9111,null,"27_16/11/2019 07:09:34","2019-11-01T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Icing found on pipes & tank of No.2 AC Reefer Compressor Unit inside AC Room","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","Refer compressor discharge pressure increased by throttling the condenser cooling outlet valve.","2019-11-25T23:59:35","","Completed","2019-11-05T23:59:35","No","No","No","Internal"]
[null,null,null,9112,null,"27_16/11/2019 07:22:08","2019-11-01T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Leak observed form flange adjacent to Main Engine Lube oil Setling Tank Outlet Valve","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Flange bolts tightened.","2019-11-25T23:59:35","","Completed","2019-11-16T23:59:35","No","No","No","Internal"]
[null,null,null,9113,null,"27_15/11/2019 1:33:36 PM","2019-11-01T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Hydraulic leak from the STBD side windlass brake cylinder","Deck - Mooring Machinery","Mooring","Equipment Related","","","","","Brake cylinder top cover seal ring and dust seal renewed-no leaks observed.","2019-11-25T23:59:35","","Completed","2019-11-17T23:59:35","No","No","No","Internal"]
[null,null,null,9114,null,"27_16/11/2019 07:07:24","2019-11-01T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Vent in AC Room - all bolts were missing","Miscellaneous","Eng. / Strg. Comp.","Behaviour Based,Human Error","","","","","Vent Frame secured with new bolts","2019-11-25T23:59:35","","Completed","2019-11-15T23:59:35","No","No","No","Internal"]
[null,null,null,9115,null,"27_16/11/2019 07:23:37","2019-11-01T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Old Valves in Engine room were not secured properly","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Behaviour Based,Human Error","","","","","Old Valves properly secured with wire","2019-11-25T23:59:35","","Completed","2019-11-17T23:59:35","No","No","No","Internal"]
[null,null,null,9116,null,"27_16/11/2019 07:25:34","2019-11-01T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Flexible pipe from Port boiler found with oil stains below the outlet","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","No.1 boiler flexible hose stain marks cleaned -no leaks observed","2019-11-25T23:59:35","","Completed","2019-11-14T23:59:35","No","No","No","Internal"]
[null,null,null,9117,null,"27_16/11/2019 07:26:46","2019-11-01T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Drums in steering gear loosely secured","Miscellaneous","Eng. / Strg. Comp.","Behaviour Based,Human Error","","","","","Drums secured properly with wire.","2019-11-25T23:59:35","","Completed","2019-11-17T23:59:35","No","No","No","Internal"]
[null,null,null,9118,null,"27_16/11/2019 07:29:16","2019-11-01T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","No.2 Aux Boiler Isolating & adjacent Valves found with Insufficient Lagging","E/R - Boiler","Eng. / Strg. Comp.","Behaviour Based,Human Error","","","","","Sufficient lagging placed and secured in place.","2019-11-25T23:59:35","","Completed","2019-11-16T23:59:35","No","No","No","Internal"]
[null,null,null,9119,null,"27_16/11/2019 08:24:00","2019-11-01T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Mesh for Soot Collectin Tank Cover found broken & missing in sections.Cover found loose","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Behaviour Based,Human Error","","","","","Mesh renewed & secured","2019-11-25T23:59:35","","Completed","2019-11-16T23:59:35","No","No","No","Internal"]
[null,null,null,9120,null,"27_16/11/2019 08:30:55","2019-11-01T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Engine Room Tank Markings/Identification missing","Miscellaneous","Eng. / Strg. Comp.","Behaviour Based,Human Error","","","","","Stenciling done as required.","2019-11-25T23:59:35","","Completed","2019-11-15T23:59:35","No","No","No","Internal"]
[null,null,null,9121,null,"27_16/11/2019 08:32:48","2019-11-01T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Engine Room Bottom Platform - The connection between the deadweight & the pedestral for lifting was disconnected","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Behaviour Based,Human Error","","","","","Deadweight & pedestral  connected","2019-11-25T23:59:35","","Completed","2019-11-14T23:59:35","No","No","No","Internal"]
[null,null,null,9122,null,"27_16/11/2019 08:21:14","2019-11-01T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Fire Extinguisher in Engine Room near Scrubber Pipe to be relocated to an accessiblelocation","LSA / FFA","Safety / LSA / FFA","Behaviour Based,Human Error","","","","","Fire Extinguisher relocated.","2019-11-25T23:59:35","","Completed","2019-11-11T23:59:35","No","No","No","Internal"]
[null,null,null,9123,null,"27_16/11/2019 07:45:25","2019-11-01T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Manifold Cover located on platform below ECR port side was not secured","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Behaviour Based,Human Error","","","","","Covers secured with proper bolts","2019-11-25T23:59:35","","Completed","2019-11-16T23:59:35","No","No","No","Internal"]
[null,null,null,9124,null,"27_16/11/2019 07:36:22","2019-11-01T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Lagging found soaked in oil underneath the platform near new Aux Generator","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Behaviour Based,Human Error","","","","","Flange tightened,cleaned and lagging painted. ","2019-11-25T23:59:35","","Completed","2019-11-12T23:59:35","No","No","No","Internal"]
[null,null,null,9125,null,"27_16/11/2019 07:31:53","2019-11-01T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Valves in Engine room for Generators found leaking from gland packing","E/R - Aux. Mach.","Eng. / Strg. Comp.","Behaviour Based,Human Error","","","","","Gland packing tightened and no leaks observed.","2019-11-25T23:59:35","","Completed","2019-11-15T23:59:35","No","No","No","Internal"]
[null,null,null,9126,null,"27_15/11/2019 2:53:25 PM","2019-11-01T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","#2 COP - pumproom - slight oil leak from the casing bolts and upper seal","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","Bolts tightened and oil cleaned.","2019-11-24T23:59:35","","Completed","2019-11-17T23:59:35","No","No","No","Internal"]
[null,null,null,9127,null,"27_15/11/2019 05:15:47","2019-11-01T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Securing Latches for AC Filter Missing in few locations","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","New latches fabricated and fitted in place","2019-11-25T23:59:35","","Completed","2019-11-17T23:59:35","No","No","No","Internal"]
[null,null,null,9128,null,"27_15/11/2019 11:19:54 AM","2019-11-01T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","3 Securing Bolts missing on Cover box of 15 ppm Bilge Separator Thermos Control Box","Critical Equip.","Eng. / Strg. Comp.","Human Error","","","","","Bolts fixed & cover box secured","2019-11-13T23:59:35","","Completed","2019-11-12T23:59:35","No","No","No","Internal"]
[null,null,null,9130,null,"27_15/11/2019 4:34:43 PM","2019-11-01T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","E/R - slight leak from the gland of the aft draft gauge valve located on the aft STBD side at bottom platform","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","gland retightened, no traces of leak.","2019-12-10T23:59:35","","Completed","2019-11-01T23:59:35","No","No","No","Internal"]
[null,null,null,9131,null,"27_16/11/2019 07:48:30","2019-11-01T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Main Engine Cylinder Lubricating System ( RPLS pump) found leaking","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","bolts retightened, no more leaks.","2019-11-25T23:59:35","","Completed","2019-11-01T23:59:35","No","No","No","Internal"]
[null,null,null,9133,null,"27_15/11/2019 11:07:39 AM","2019-11-01T23:59:35","Critical Equipment,Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Air Leak in CCR IG Panel Cabinet","Inert Gas","Cargo / Ballast Systems","Equipment Related","","","","","Vent valve eased up and flow regulation adjusted for less purging of air","2019-11-25T23:59:35","","Completed","2019-11-17T23:59:35","No","No","No","Internal"]
[null,null,null,9134,null,"27_15/11/2019 4:23:34 PM","2019-11-01T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Steering gear room - Fireman locker needs proper securing arrangement\t","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","Proper securing arrangement made","2019-12-10T23:59:35","","Completed","2019-11-21T23:59:35","No","No","No","Internal"]
[null,null,null,9135,null,"27_16/11/2019 06:37:41","2019-11-01T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Indicator Lamp for Hi-Hi & VECS panel Power Button not working","Miscellaneous","Cargo / Ballast Systems","Equipment Related","","","","","Indicator Lamp is working for Hi-Hi & VECS ppower panel.","2019-11-25T23:59:35","","Completed","2019-11-22T23:59:35","No","No","No","Internal"]
[null,null,null,9136,null,"27_15/11/2019 4:31:11 PM","2019-11-01T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","E/R - lower/upper plunger for the level indicator for some of the tanks was found in stuck position. E.g. EGB soot tank, hyd tank for aft mooring, hot well tank etc","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Gauge glass isolating valves eased up.","2019-12-26T23:59:35","","Completed","2019-11-22T23:59:35","No","No","No","Internal"]
[null,null,null,9137,null,"27_16/11/2019 07:18:47","2019-11-01T23:59:35","Critical Equipment,Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Open/Shut Indicator for Central Cooler B/V High Seachest / Low Seachest not Working","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Limit switches rebnewed-working satisfactory.","2019-11-25T23:59:35","","Completed","2019-11-17T23:59:35","No","No","No","Internal"]
[null,null,null,9138,null,"27_16/11/2019 10:30:51 AM","2019-11-01T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","CCR - The bulb for the power indicator for Hi-Hi level alarm panel is not working. As a result it cannot be made out if the panel is in or off.","Cargo Mach.,Elect. Mach. & Equip.","Cargo / Ballast Systems","Equipment Related","","","","","Power indicator lamp is working","2020-01-26T23:59:35","","Completed","2019-11-21T23:59:35","No","No","No","Internal"]
[null,null,null,9139,null,"27_15/11/2019 4:33:13 PM","2019-11-01T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","E/R - flow indicator for automatice air control unit for aft seal & S/T was found to be opaque.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Flow indicator glass cleaned up.","2019-12-26T23:59:35","","Completed","2019-11-25T23:59:35","No","No","No","Internal"]
[null,null,null,9142,null,"27_15/11/2019 4:28:22 PM","2019-11-01T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","E/R - bottom platform some of the securing screws for the platform plates ae missing","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","To secure all the platform plates with screws","2019-12-10T23:59:35","","Completed","2019-11-13T23:59:35","No","No","No","Internal"]
[null,null,null,9143,null,"27_16/11/2019 08:18:12","2019-11-01T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Lower Bearing Temperature for No.3 COP was bserved high during discharging compared to No.1 & No.2 COP","Cargo Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","New grease replaced and will observe temp rise during discharge.","2019-11-25T23:59:35","","Completed","2019-11-26T23:59:35","No","No","No","Internal"]
[null,null,null,9144,null,"27_16/11/2019 08:16:13","2019-11-01T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Upper Pump Bearing Temperature for COP 1 was observed high during Discharging compared to COP 2 & 3","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","Grease replaced and will observe temp.rise during discharge.","2019-11-25T23:59:35","","Completed","2019-11-26T23:59:35","No","No","No","Internal"]
[null,null,null,9147,null,"27_16/11/2019 10:36:49 AM","2019-11-01T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","The duty mess room bulkheads were dirty with oil/grease stain on bulkhead in some locations.","Accommodation","General Appearance","Human Error","","","","","Bulkheads cleaned","2019-12-26T23:59:35","","Completed","2019-12-01T23:59:35","No","No","No","Internal"]
[null,null,null,9148,null,"27_16/11/2019 07:15:25","2019-11-01T23:59:35","Critical Equipment,Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","3 Light shades in Engine Room were found broken or securing clamps Missing","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","Light shades renewed and Securing Clamps repaired","2019-11-25T23:59:35","","Completed","2019-12-01T23:59:35","No","No","No","Internal"]
[null,null,null,9151,null,"27_16/11/2019 06:33:47","2019-11-01T23:59:35","Critical Equipment,Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","No.1 Cargo Line Pressure Gauge not Working in CCR","Miscellaneous","Cargo / Ballast Systems","Equipment Related","","","","","Cargo line to the pressure transmitter found choked and same claered.Pr.transmitter calibrated and compared raed out with the gauge in CCR-all in ordeer.","2019-11-25T23:59:35","","Completed","2019-12-05T23:59:35","No","No","No","Internal"]
[null,null,null,9152,null,"27_15/11/2019 2:04:35 PM","2019-11-01T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","LSMGO line manifold marking missing. Some flange bolts are short in length. Drain pipe and vent pipe located on top has valve fitted but no blank.","Deck - Pipe / Fittings","MARPOL Related","Equipment Related","","","","","LSMGO Bunker line stenciled.Blank plugs installed \n\nand valve flange  small bolts replaced with longer ones.","2019-11-25T23:59:35","","Completed","2019-11-27T23:59:35","No","No","No","Internal"]
[null,null,null,9157,null,"27_15/11/2019 1:43:34 PM","2019-11-01T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Slight vapour leak from 3C and 5C COT PV valve vacuum side","Deck - Pipe / Fittings,Hull & Tanks","MARPOL Related","Equipment Related","","","","","SEAT CLEANED AND ADJUSTED, NO MORE LEAKING","2019-11-25T23:59:35","","Completed","2019-11-20T23:59:35","No","No","No","Internal"]
[null,null,null,9158,null,"27_16/11/2019 10:24:09 AM","2019-11-01T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","CCR - No1 manifold pressure gauge not working","Cargo Mach.,Elect. Mach. & Equip.","Cargo / Ballast Systems","Equipment Related","","","","","NO 1 MANIFOLD PRESS GAUGE / TRANSMITER NEAR NO1 CARGO LINE AT MIDSHIP CALIBRATED, LINE BLOWN THROUGH, PRESSURE READING COMPAIRED WITH CCR GAUGE, IDENTICAL READING OBSERVED.","2019-12-26T23:59:35","`","Completed","2019-12-05T23:59:35","No","No","No","Internal"]
[null,null,null,9159,null,"27_16/11/2019 10:27:32 AM","2019-11-01T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","CCR - Continiuous alarm in the anemometer located in CCR. Once it is switched OFF, cannot be switched ON easily.","Elect. Mach. & Equip.","Cargo / Ballast Systems","Equipment Related","","","","","old anemometer unit showing ok now no more alarm, vessel received new anemometer on 23/11/2019 at galle. If old unit showing malfunction again we will renew.","2020-01-26T23:59:35","","Completed","2019-11-13T23:59:35","No","No","No","Internal"]
[null,null,null,9160,null,"27_16/11/2019 10:39:11 AM","2019-11-01T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Proper securing arrangement to be made for the weights in gymnasium.","Accommodation ,Miscellaneous","General Appearance","Equipment Related","","","","","All weights are properly secured in weight stag and weight stag is properly secured with the bulkhead","2019-12-26T23:59:35","","Completed","2019-11-14T23:59:35","No","No","No","Internal"]
[null,null,null,9161,null,"27_16/11/2019 10:34:34 AM","2019-11-01T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","The D-Link box located in the DT & CT locker room located opposite side of the CCR was kept loose.","Elect. Mach. & Equip.","Communication","Equipment Related","","","","","Box removed from the cabinet and secured in poop deck bosun store.","2020-01-26T23:59:35","","Completed","2019-11-17T23:59:35","No","No","No","Internal"]
[null,null,null,9162,null,"27_15/11/2019 1:57:47 PM","2019-11-01T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","STBD side hose handling crane's hydraulic hoses are not secured/bunched together","Deck - Machinery","General Appearance","Equipment Related","","","","","All secured/bunched together with cable tie","2019-11-25T23:59:35","","Completed","2019-11-22T23:59:35","No","No","No","Internal"]
[null,null,null,9163,null,"27_15/11/2019 2:13:59 PM","2019-11-01T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","STBD side bridge wing - manouevring console has debris located inside the covering","Navigation - Others","Navigation","Equipment Related","","","","","cleaned the console, all debris dust removed","2019-11-10T23:59:35","","Completed","2019-11-14T23:59:35","No","No","No","Internal"]
[null,null,null,9164,null,"27_15/11/2019 2:23:47 PM","2019-11-01T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","STBD side liferaft latest inspection date done on Sep 2019 label missing.","LSA / FFA","Safety / LSA / FFA","Human Error,Inappropriate Procedure","","","",""," labelled/marked, job done","2019-11-25T23:59:35","","Completed","2019-11-20T23:59:35","No","No","No","Internal"]
[null,null,null,9165,null,"27_16/11/2019 06:35:58","2019-11-01T23:59:35","Critical Equipment,Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Anemometer in CCR showing error ","Navigation - Others","Navigation","Equipment Related","","","","","Old anemometer now working fine with no alarm, recvd new set at galle","2019-11-25T23:59:35","","Completed","2019-11-13T23:59:35","No","No","No","Internal"]
[null,null,null,9166,null,"27_16/11/2019 06:39:17","2019-11-01T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","D-Link box in A Deck Duct not secured","Navigation - Others","Communication","Behaviour Based,Human Error","","","","","Box secured in poop deck bosun store","2019-11-25T23:59:35","","Completed","2019-11-17T23:59:35","No","No","No","Internal"]
[null,null,null,9167,null,"27_16/11/2019 06:42:20","2019-11-01T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","No proper securing arrangement for weights in Gymnasium ","Miscellaneous","MLC Related","Behaviour Based,Human Error","","","","","Fabrication of secured arrangement done, now secured","2019-11-25T23:59:35","","Completed","2019-11-14T23:59:35","No","No","No","Internal"]
[null,null,null,9168,null,"27_15/11/2019 2:26:07 PM","2019-11-01T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Some of SI lights for the lifebuoys had all the markings missing, including expiry date etc.","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","Missing details posted","2019-11-25T23:59:35","","Completed","2019-11-20T23:59:35","No","No","No","Internal"]
[null,null,null,9169,null,"27_15/11/2019 2:43:15 PM","2019-11-01T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Observation tank for the slop tank steam coils - the glass view has been blanked.\n\nThe observation tank has to be covered in canvas.\n\nAlso one bolt for the retainer ring is missing.","Deck - Machinery,Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","","","","","Glass view blkank  reomved.\n\nTo be covered with canvas when not in use.\n\nOne missing  bolt fitted in place","2019-11-25T23:59:35","","Completed","2019-11-09T23:59:35","No","No","No","Internal"]
[null,null,null,9170,null,"27_15/11/2019 2:09:49 PM","2019-11-01T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Elecator escape/maintenance hatches on PORT side bridge wing has no markings","Miscellaneous","Emgcy. Systems","Inappropriate Procedure","","","","","stencilling done","2019-11-25T23:59:35","","Completed","2019-11-22T23:59:35","No","No","No","Internal"]
[null,null,null,9171,null,"27_15/11/2019 2:57:03 PM","2019-11-01T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Pumproom - slight oil leak from the glands of the stripping pump","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","Leakage arrested ","2019-11-25T23:59:35","","Completed","2019-11-23T23:59:35","No","No","No","Internal"]
[null,null,null,9172,null,"27_15/11/2019 4:21:45 PM","2019-11-01T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Steering gear room - Hyd oil tank for mooring - evidence of slight leak from the lvel indicator. Also the lower plunger valve was stuck in open position.","Deck - Mooring Machinery","Eng. / Strg. Comp.","Equipment Related","","","","","Leakage rectified by renewing the o-rings.","2019-12-10T23:59:35","","Completed","2019-12-11T23:59:35","No","No","No","Internal"]
[null,null,null,9176,null,"27_16/11/2019 07:11:24","2019-11-01T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Indications of leak from the seal of Low Expansion foam pump","Critical Equip.,LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","Currently no leaks observed.","2019-11-25T23:59:35","","Completed","2019-12-19T23:59:35","No","No","No","Internal"]
[null,null,null,9177,null,"27_15/11/2019 2:47:08 PM","2019-11-01T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Port side windlass - the wheel for the disk brake should be covered as same has been decommissioned","Deck - Machinery","Mooring","Equipment Related","","","","","AS THE BRAKE DRUM ROTATING WITH THE ROTATION OF GYPSY AND WINCH DRUM HENCE CAN NOT BE COVERED","2019-11-25T23:59:35","","Completed","2019-12-19T23:59:35","No","No","No","Internal"]
[null,null,null,9179,null,"27_15/11/2019 2:50:38 PM","2019-11-01T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Pumproom davit located outside pumproom entrance has all the gears exposed - cover is missing","Deck - Machinery","Emgcy. Systems","Equipment Related","","","","","Cover  fitted on exposed gears","2019-11-25T23:59:35","","Completed","2019-12-21T23:59:35","No","No","No","Internal"]
[null,null,null,9180,null,"27_15/11/2019 05:35:59","2019-11-01T23:59:35","Critical Equipment","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","Alrams Active on No.1 & No.2 UPS on Bridge","Critical Equip.,Elect. Mach. & Equip.","Emgcy. Systems","Equipment Related","","","",""," NO 1 UPS RENEWED BY SHORE TECHNICIAN AT SINGAPORE AND ALL FOUND TO BE IN ORDER.","2019-11-25T23:59:35","","Completed","2019-12-21T23:59:35","No","No","No","Internal"]
[null,null,null,9181,null,"27_16/11/2019 07:47:04","2019-11-01T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Main Engine Aft Scavanage air Cooler - Forward end was found leaking","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Defect deferred to DD and Refman made for the same","2019-11-25T23:59:35","","Completed","2019-12-21T23:59:35","No","No","No","Internal"]
[null,null,null,9183,null,"27_16/11/2019 06:22:34","2019-11-01T23:59:35","Critical Equipment,Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Fire Line Pressure Gauge in CCR showing Erratic Reading","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","Pressure transmitter needs renewal.Will raise RO for the same.","2019-11-25T23:59:35","","Completed","2019-12-21T23:59:35","No","No","No","Internal"]
[null,null,null,9185,null,"27_16/11/2019 10:13:37 AM","2019-11-01T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","CCR - Stroke indicator for stripper pump is not showing the correct stroke value at times - same to be further investigated","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","To be investigated.","2019-12-26T23:59:35","","Completed","2019-12-21T23:59:35","No","No","No","Internal"]
[null,null,null,9186,null,"27_16/11/2019 10:10:13 AM","2019-11-01T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","CCR - Draught gauge not showing correct draughts","Miscellaneous","Navigation","Equipment Related","","","","","Shore technician expects to attend V/L at Zhoushan about 28th Dec.2019","2019-12-26T23:59:35","","Completed","2019-12-21T23:59:35","No","No","No","Internal"]
[null,null,null,9187,null,"27_16/11/2019 10:19:00 AM","2019-11-01T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","CCR - 2nd hydraulic pump does not cut-in automatically when the pressure in the system drops below the set value.","Deck - Machinery","Cargo / Ballast Systems","Equipment Related","","","","","Will raise RO in Jan'20","2020-01-26T23:59:35","","Completed","2019-12-21T23:59:35","No","No","No","Internal"]
[null,null,null,9188,null,"27_16/11/2019 10:15:58 AM","2019-11-01T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp."," - gas flow sensor for fixed gsa detection system was bypassed. Spares have been received - same to be fixed back in place","Cargo Mach.,Elect. Mach. & Equip.","Cargo / Ballast Systems","Equipment Related","","","","","2Nos.Mist catcher renewed.New Gas pump fitted in place,tried out and found to be turning hard.On further investigation ,motor winding found to be open ckted.Will land pump with the supplier at Singapore about 10th Jan 2020.","2019-12-26T23:59:35","","Completed","2019-12-21T23:59:35","No","No","No","Internal"]
[null,null,null,9074,null,"27_Mon Nov 11 2019 18:45:27 GMT+0000 (Coordinated Universal Time)","2019-11-03T23:59:35","","Ship Staff","Ship Staff Insp.","AHU NO.1 AND 2  FRESH AIR INTAKE FLAPS SEIZED AND OPERATING LINKAGE BROKEN","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","FLAPS MADE FREE AND LINKAGES REPAIRED","2019-11-05T23:59:35","","Completed","2019-11-03T23:59:35","No","No","No","Internal"]
[null,null,null,9075,null,"27_13/11/2019 10:34:55 AM","2019-11-03T23:59:35","Other","Ship Staff","Ship Staff Insp.","SCRUBBER PUMP OVERBOARD LINE LEAKING FROM THE WELD JOINT","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","CORRODED/WASTED PIPE (L-1000MM X NB-350MM|) RENEWED WITH A GALVANISED AND EPOXY COATED PIPE.","2019-11-10T23:59:35","","Completed","2019-11-07T23:59:35","No","No","No","Internal"]
[null,null,null,9078,null,"27_13/11/2019 11:07:48 AM","2019-11-03T23:59:35","Other","Ship Staff","Ship Staff Insp.","A/E2 CHARGE AIR TEMP.SENSOR GIVING ERRATIC READ OUT.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","SENSOR RENEWED - WORKING SATISFACTORY","2019-11-11T23:59:35","","Completed","2019-11-03T23:59:35","No","No","No","Internal"]
[null,null,null,9079,null,"27_13/11/2019 2:02:42 PM","2019-11-04T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","One of the limit switch in stbd side davit was not working, its contacts are damaged due the weather condition\t\t","Deck - Machinery","Safety / LSA / FFA","External Factors","","","","","Switch renewed with the spare one after repairing the base plate.","2019-11-11T23:59:35","","Completed","2019-11-05T23:59:35","No","No","No","Internal"]
[null,null,null,2548,null,"27_15/10/2019 8:26:56 AM","2019-11-10T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","HFO Purifier no.1 temperature control valve not functioning in Auto mode","E/R - Purifier","Eng. / Strg. Comp.","Equipment Related","10.2","Low","","","Temp.controller renewed","2020-01-26T23:59:35","DLOT190064","Completed","2020-02-29T23:59:35","No","No","No","Internal","At DD in Oct, these were repaired but again trouble persisted, spares arranged at Singapore 28th Feb."]
[null,null,null,9140,null,"27_30/11/2019 1:49:15 PM","2019-11-20T23:59:35","Other","Ship Staff","Ship Staff Insp.","Vaccum condenser sea water pipe(flanged elbow) after the outlet valve leaking","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","New pipe fabricated (NB 500mmx 1200m Length) ,2 coats of epoxy applied and fitted in place.","2019-12-10T23:59:35","","Completed","2019-11-24T23:59:35","No","No","No","Internal"]
[null,null,null,9141,null,"27_30/11/2019 1:54:09 PM","2019-11-21T23:59:35","Other","Ship Staff","Ship Staff Insp.","Sea water inlet  pipe to cooler for Aft hyd.mooring system leaking from the weld seam.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Pipe welded at the weld seam and fitted back in place.Tried out-no leaks.","2019-12-18T23:59:35","","Completed","2019-11-25T23:59:35","No","No","No","Internal"]
[null,null,null,9145,null,"27_Fri Apr 12 2019 13:43:52 GMT+0000 (Coordinated Universal Time)","2019-11-26T23:59:35","Other","Ship Staff","Ship Staff Insp.","M/E Unit no.3 and 7 local exh.gas temp.gauge defective.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Temperature gauges renewed.","2019-12-15T23:59:35","","Completed","2019-11-28T23:59:35","No","No","No","Internal"]
[null,null,null,9146,null,"27_Wed Dec 04 2019 13:52:44 GMT+0000 (Coordinated Universal Time)","2019-11-26T23:59:35","Other","Ship Staff","Ship Staff Insp.","M/E RPSL Pump no.2 tripping on overload.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Pump and motor overhauled.Now it is operating satisfactory.","2019-12-15T23:59:35","","Completed","2019-11-29T23:59:35","No","No","No","Internal"]
[null,null,null,9153,null,"27_Sat Oct 12 2019 20:16:46 GMT+0000 (Coordinated Universal Time)","2019-11-27T23:59:35","Other","Ship Staff","Ship Staff Insp.","A/Es fuel oil heater no.1 leaking from the end cover gasket","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Heater cleaned and end cover gasket renewed.","2019-12-23T23:59:35","","Completed","2019-12-01T23:59:35","No","No","No","Internal"]
[null,null,null,9154,null,"27_Sat Oct 12 2019 20:20:52 GMT+0000 (Coordinated Universal Time)","2019-11-28T23:59:35","","Ship Staff","Ship Staff Insp.","Aux.boiler no.2 main steam stop valve bonnet gasket passing.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Bonnet gasket renewed.","2019-12-25T23:59:35","","Completed","2019-12-03T23:59:35","No","No","No","Internal"]
[null,null,null,9155,null,"27_Sat Oct 12 2019 20:24:37 GMT+0000 (Coordinated Universal Time)","2019-11-28T23:59:35","Other","Ship Staff","Ship Staff Insp.","A/Es fuel oil heater no.2 leaking from the end cover gasket","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Heater cleaned and end cover gasket renewed.","2019-12-26T23:59:35","","Completed","2019-12-04T23:59:35","No","No","No","Internal"]
[null,null,null,9156,null,"27_Thu Dec 12 2019 07:56:06 GMT+0000 (Coordinated Universal Time)","2019-11-29T23:59:35","Other","Ship Staff","Ship Staff Insp.","Aux.Boiler's fuel oil pump no.2 mech seal leaking.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Pump seal renewed and electric motor o,hauled.","2019-12-26T23:59:35","","Completed","2019-12-06T23:59:35","No","No","No","Internal"]
[null,null,null,9070,null,"27_23/12/2019 6:14:06 PM","2019-12-16T23:59:35","Other","Ship Staff","Ship Staff Insp.","Scruuber overboard pipe observed to be partly clogged.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Overboard valve closed and oboard pipe drained off water.Removed NRV from place which was found to be fully clogged with polyeuthrene coating.Scrubber pump tried out -satisfactory.","2020-01-26T23:59:35","","Completed","2020-01-01T23:59:35","No","No","No","Internal"]
[null,null,null,9173,null,"27_21/12/2019 1:57:12 PM","2019-12-16T23:59:35","Other","Ship Staff","Ship Staff Insp.","A/E 2 fuel oil inlet temp.sensor faulty.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Sensor cleaned and observed to be functioning satisfactory","2020-03-26T23:59:35","","Completed","2019-12-18T23:59:35","No","No","No","Internal"]
[null,null,null,9174,null,"27_25/12/2019 6:19:41 AM","2019-12-16T23:59:35","Other","Ship Staff","Ship Staff Insp.","AEs Fuel oil heater end cover gasket leaking","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Heaters removed from place,cleaned up and end cover gasket renewed.","2019-12-26T23:59:35","","Completed","2019-12-18T23:59:35","No","No","No","Internal"]
[null,null,null,9175,null,"27_25/12/2019 6:23:36 AM","2019-12-18T23:59:35","Other","Ship Staff","Ship Staff Insp.","IG scrubber sea water inlet valve from deck seal pump leaking.","Inert Gas","Eng. / Strg. Comp.","Equipment Related","","","","","Valve renewed with a spare one.","2019-12-26T23:59:35","","Completed","2019-12-19T23:59:35","No","No","No","Internal"]
[null,null,null,9601,null,"27_05/01/2020 4:23:43 PM","2019-12-27T23:59:35","Other","Ship Staff","Ship Staff Insp.","LT Cooler no.2 sea water inlet valve leaking from the valve body.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Valave replaced with the new one.","2020-01-26T23:59:35","","Completed","2019-12-27T23:59:35","No","No","No","Internal"]
[null,null,null,9602,null,"27_07/01/2020 4:44:48 PM","2019-12-30T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Hot water calorifier electric motor making abnormal noise.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Motor dismantled,inspected and bearings renewed.","2020-01-25T23:59:35","","Completed","2019-12-30T23:59:35","No","No","No","Internal"]
[null,null,null,9603,null,"27_14/01/2020 9:55:58 AM","2019-12-30T23:59:35","Other","Ship Staff","Ship Staff Insp.","Main engine jacket water pre-heating pump motor making abnormal noise","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Motor o'hauled with new bearings.","2020-03-31T23:59:35","","Completed","2019-12-31T23:59:35","No","No","No","Internal"]
[null,null,null,9596,null,"27_05/01/2020 4:29:16 PM","2019-12-31T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Capacitors  to disconnected/remove for the LED light fittings in the engine room and accomodation","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","11.13","Low","","","Capacitors removed and LED lights renewal job  completed 95%.Will complete the rest in the next 2 days.","2020-06-25T23:59:35","DLOT200097 applies","Completed","2020-06-10T23:59:35","No","No","No","Internal"]
[null,null,null,9600,null,"27_14/01/2020 10:00:04 AM","2020-01-05T23:59:35","Other","Ship Staff","Ship Staff Insp.","Harbour sea water pump leaking from the mechanical seal","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.31","Very High","","","Mech.seal cover opened up ,stationary and rotary seal surface cleaned up and spring eased up.\n\n","2020-04-04T23:59:35","","Completed","2020-01-22T23:59:35","No","No","No","Internal"]
[null,null,null,9597,null,"27_14/01/2020 10:05:54 AM","2020-01-06T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Exhaust gas scrubber sea water pump no.2 mech.seal leaking","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.31","Very High","","","Mech.seal renewed.","2020-06-25T23:59:35","Seal received under Guarantee claim.","Completed","2020-05-01T23:59:35","No","No","No","Internal"]
[null,null,null,9598,null,"27_14/01/2020 10:08:30 AM","2020-01-06T23:59:35","Defect","Ship Staff","Ship Staff Insp.","IGS Scrubber pump mech.seal leaking","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Mech.seal renewed","2020-04-06T23:59:35","","Completed","2020-01-11T23:59:35","No","No","No","Internal"]
[null,null,null,9599,null,"27_14/01/2020 11:01:44 AM","2020-01-07T23:59:35","Defect","Ship Staff","Ship Staff Insp.","IGS Deck seal pump no.1 mech.seal leaking","E/R - Pumps,Inert Gas","Eng. / Strg. Comp.","Equipment Related","8.27","Medium","","","Mech.seal renewed","2020-04-06T23:59:35","","Completed","2020-01-19T23:59:35","No","No","No","Internal"]
[null,null,null,10183,null,"27_28/01/2020 2:02:31 PM","2020-01-16T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","VRCS - Load/Unload pump operations reported erratic, sometimes require 2 pumps to maintain pressure","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.8","Medium","","","Hyd.pump cut in /cut off relay replaced and operation observed to be satisfactory. ","2020-09-25T23:59:35","","Completed","2020-06-23T23:59:35","No","No","No","Internal"]
[null,null,null,10184,null,"27_28/01/2020 2:07:34 PM","2020-01-16T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Cargo manifold - Main valve #2 suspected leaking","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.6","Medium","","","Valve along with the pipe section removed from place.Valve brought to E/R w/shop ,seat ring dismantled and new seat ring fitted.Valve tested with air and water for any leakage-Satisfactory.","2020-01-25T23:59:35","","Completed","2020-01-24T23:59:35","No","No","No","Internal"]
[null,null,null,10185,null,"27_28/01/2020 2:10:06 PM","2020-01-16T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Mooring winches - Brake band stopper bolts – most of them hardly any clearance observed (bolts painted over)","Deck - Mooring Machinery","Mooring","Equipment Related","9.15","Medium","","","To adjust all bolts with min 3 mm gap and keep the bolts greased. All bolts in FWD and AFT mooring winches attained, old paint removed from the bolts, lubricated and adjusted to 3 mm gap between brake band and stopper bolts.  ","2020-01-26T23:59:35","","Completed","2020-01-25T23:59:35","No","No","No","Internal"]
[null,null,null,10186,null,"27_28/01/2020 2:11:56 PM","2020-01-16T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","SIP vents - Most of them noticed with scattered rusts","Miscellaneous","Structural Condn. / WT integrity ","Equipment Related","11.7","High","","","To derust and paint. Started derusting and painting, work in progress. BY 17-FEB-2020 85% JOB COMPLETED. JOB DONE. ","2020-02-15T23:59:35","","Completed","2020-02-15T23:59:35","No","No","No","Internal"]
[null,null,null,10187,null,"27_28/01/2020 2:13:32 PM","2020-01-16T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Lifeboat davits - Davit structires noticed with rust weepings and scattered spot rusts","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.28","Very High","","","To derust and paint. Work In progress. BY 17-FEB-2020 STBD SIDE DEVIT DERUSTED AND PAINTED. PORT SIDE DEVIT DERUSTING JOB COMPLETED, PAINTING IN PROGRESS. JOB DONE.","2020-02-06T23:59:35","","Completed","2020-02-15T23:59:35","No","No","No","Internal"]
[null,null,null,10188,null,"27_28/01/2020 2:15:40 PM","2020-01-16T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Accommodation block - Bridge/accomm front, port hole sills have rust/weepings","Accommodation","Structural Condn. / WT integrity ","Equipment Related","11.6","Medium","","","Full accomm/bridge front needs spot derusting and complete coat of paint. ON 29 FEB 2020 JOB STARTED, TRY TO COMPLETE BY 3-4 DAYS TIME, WX PERMITS. job completed on 07-Mar-2020","2020-03-16T23:59:35","","Completed","2020-03-02T23:59:35","No","No","No","Internal"]
[null,null,null,10189,null,"27_28/01/2020 2:20:40 PM","2020-01-16T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","IG system - Reported 4S and few other tanks IG valves, gear operating mechanism tight and few had cracked","Deck - Pipe / Fittings,Hull & Tanks","Cargo / Ballast Systems","Equipment Related","8.2","Medium","","","To order Gear mechanism and replace same. REQUISITION RAISED IN PAL (REQ NO:  DLOT200061), BY 29 FEB 2020 STILL AWAITING FOR SUPPLY, ALSO  STARTED OVERHAULING THE V/Vs AND WORM GEAR MECHANISM. WILL UPDATE REPORT OF HOW MANY WE CAN MAKE FULLY OPERATIONAL AFTER OVERHAULING. After overhauling the gear it looks like worm gear is not the prob but v/v flaps are fully tight. Need to overhaul the valve flaps which may be struck due to carbon deposit. RO RAISED.                                                  - As per supdt job raised in REFMAN for drydock","2020-07-26T23:59:35","RO DLOT 200061 / 200103 / 200104                          As per supdt job raised in REFMAN for dryd","Completed","2020-06-10T23:59:35","No","No","No","Internal"]
[null,null,null,10190,null,"27_28/01/2020 2:23:11 PM","2020-01-16T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Foam Monitor - Few Monitor’s gun holding springs broken","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.35","Medium","","","To order new springs. Req raised on 30-Jan-2020, Req no( DLOT 200052)                                  -Item received on 05.05.2020 at singapore.  same has been renewed on 07.05.2020","2020-02-15T23:59:35","Req no( DLOT 200052)                                  ","Completed","2020-04-02T23:59:35","No","No","No","Internal"]
[null,null,null,10191,null,"27_28/01/2020 2:25:46 PM","2020-01-16T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Load Cell - Reported not on board","Deck - Machinery","Cargo / Ballast Systems","Equipment Related","8.5","Very High","","","To check again and liaise with procure dept, this should be there onbd , for Hose cranes to be load tested prior arrival for cargo ops/Port. LOAD CELL FOUND ONBOARD.","2020-02-15T23:59:35","","Completed","2020-02-02T23:59:35","No","No","No","Internal"]
[null,null,null,10192,null,"27_28/01/2020 2:28:17 PM","2020-01-16T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Deck Pipe stacks - Pipe under supports observed rust on 30% of pipe supports","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.4","Very High","","","To attempt immediately and ensure thy are derusted and maintained rust free . ON 29 FEB2020 JOB RESUMED AGAIN IN THE MANIFOLD AREA PIPE STACK AS DISCUSSED WITH TECH. SUPDT.                                             -BY 15-MAR-20 MANIFOLD ACROSS PIPE STACK CHIPPING AND PAINTING COMPLETED                 - NOW CHIPPING STARTED MANIFOLD TO AFT PIPE STACK AREA","2020-03-15T23:59:35","","Completed","2020-03-10T23:59:35","No","No","No","Internal"]
[null,null,null,10193,null,"27_28/01/2020 2:30:41 PM","2020-01-16T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Main Deck - Weekly high pressure deck wash not carried out","Miscellaneous","General Appearance","Inappropriate Procedure","11.3","Medium","","","The regime not to be missed, which shall take care of corrosion control to a great extent","2020-01-23T23:59:35","","Completed","2020-02-08T23:59:35","No","No","No","Internal"]
[null,null,null,10194,null,"27_28/01/2020 2:32:40 PM","2020-01-16T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","AE #3 - Fuel lines were observed externally dirty","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","To clean the lagging/insulation and maintain stain free","2020-01-23T23:59:35","","Completed","2020-01-23T23:59:35","No","No","No","Internal"]
[null,null,null,10195,null,"27_28/01/2020 4:07:55 PM","2020-01-16T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Boiler uptake - Water leakage signs/heavy rust stains on the aft side of Boiler funnel uptake from top most funnel deck till C deck","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","It  happened due to bloackage of drain pipe at the funnel top deck.Painting /cleaning carried out as required till C deck","2020-01-25T23:59:35","","Completed","2020-01-24T23:59:35","No","No","No","Internal"]
[null,null,null,10196,null,"27_28/01/2020 4:12:08 PM","2020-01-16T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Steam line - Leak through lagging noticed abobe TG condenser, line going to AE3 FCU \t","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Leakage rectified.","2020-01-23T23:59:35","","Completed","2020-01-23T23:59:35","No","No","No","Internal"]
[null,null,null,10197,null,"27_28/01/2020 4:13:43 PM","2020-01-16T23:59:35","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","AE #1- Falling due for decarb","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Riding team for A/E1 overhaul joined at Galle on 13th Feb.2020 late evening and job completed on 19th Feb 2020.Gen.tried out and found to be working satisfactory.","2020-01-23T23:59:35","","Completed","2020-02-14T23:59:35","No","No","No","Internal"]
[null,null,null,10198,null,"27_28/01/2020 4:16:58 PM","2020-01-16T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Control air comp - Decommissioned compressor lying in MAC platform","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Compressor removed from place and kept ready for landing","2020-03-16T23:59:35","","Completed","2020-03-06T23:59:35","No","No","No","Internal"]
[null,null,null,10199,null,"27_28/01/2020 2:22:12 PM","2020-01-16T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","COW lines - COW lines observed rusted heavily","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.34","High","","","To attend to all COW lines – if any lines are suspected of thinning down, to include in REFFMAN. Chipping and painting job already in progress near 1ws cot area and  job progress identified during supdt visit,  following supdt's instruction to complete F'castle to 1ws cot  thorough full chipping and full top coat painting 1st before reaching load port. COW lines in that area already been attended. others already planned to carry out. BY 17 FEB 2020 AFT OF MANIFOLD AREA TO 4WS COT AREA ALREADY COMPLETED. BY 29 FEB2020 JOB RESUMED AGAIN.                                                                   - BY 15-MAR-20 FWD TO 4C COT AREA ALL COW LINE MAINTENANCE COMPLETED, 5 ws and slop ws are in progress.                                         -By 12-Apr-20 only SLop wings Cow lines left rest all complete                                                                                     - All done, job complete","2020-04-25T23:59:35","","Completed","2020-04-20T23:59:35","No","No","No","Internal"]
[null,null,null,10200,null,"27_28/01/2020 4:19:18 PM","2020-01-16T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","PORT sea chest - Steam blow line connected to sea chest – has no support danger of shearing if heavy weight/or some one stands on top","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.31","Very High","","","Steam blow pipe properly supported.","2020-02-16T23:59:35","","Completed","2020-01-24T23:59:35","No","No","No","Internal"]
[null,null,null,10201,null,"27_28/01/2020 4:21:02 PM","2020-01-16T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Scrubber - Exhaust pipe from ER funnel to scrubber deck/tower – insulation sheet had started rusting","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.19","Very High","","","Pipe cleaned and painted with a heat resistant paint.","2020-01-31T23:59:35","","Completed","2020-02-23T23:59:35","No","No","No","Internal"]
[null,null,null,10202,null,"27_28/01/2020 4:24:29 PM","2020-01-16T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Scrubber Tower - Scrubber tower's D deck and C deck door has no lock from inside against unauthorized entry (ISPS) – bottom deck entry door can be locked from outside","Miscellaneous","Eng. / Strg. Comp.","Inappropriate Procedure","7.4","Low","","","Arrangement made to locck the Sox.scrubber doors from inside.","2020-01-31T23:59:35","","Completed","2020-01-24T23:59:35","No","No","No","Internal"]
[null,null,null,10203,null,"27_28/01/2020 4:26:22 PM","2020-01-16T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","IG scrubber - IG scrubber inlet pipe (to paint) outer lagging sheet corroded/rusted","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.19","Very High","","","Pipe cleaned and painted","2020-02-16T23:59:35","","Completed","2020-02-23T23:59:35","No","No","No","Internal"]
[null,null,null,10204,null,"27_28/01/2020 4:39:22 PM","2020-01-16T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Spares Inventory - Still pending to be fully updated in PAL","Documentation","Cert. & Docu.","Human Error","10.21","Medium","","","It is the repeated defect,hence closing out.","2020-03-20T23:59:35","","Completed","2020-04-08T23:59:35","No","No","No","Internal"]
[null,null,null,10205,null,"27_28/01/2020 4:37:52 PM","2020-01-16T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","PMS - Spares consumption reporting in PAL, is still lacking","Documentation","Cert. & Docu.","Human Error","10.21","Medium","","","Spares consumption are updated on all overhaul Jobs.","2020-01-26T23:59:35","","Completed","2020-01-23T23:59:35","No","No","No","Internal"]
[null,null,null,10209,null,"27_28/01/2020 4:35:54 PM","2020-01-16T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Funnel platforms - Floor plates/gratings – additional – lying loose if Funnel deck (below the damper valve deck)","Miscellaneous","Eng. / Strg. Comp.","Human Error","10.29","Medium","","","To remove all gratings/plates lying lose and check all decks again for any loose/ additional items. All gratings and plates lashed with wire no loose gratings are in place.","2020-01-31T23:59:35","","Completed","2020-01-27T23:59:35","No","No","No","Internal"]
[null,null,null,10210,null,"27_28/01/2020 2:34:29 PM","2020-01-16T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","AE #3 - LO leakage observed on the block next to cylinder heads – Gov side","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","To check source of leakage and arrest","2020-01-18T23:59:35","","Completed","2020-01-17T23:59:35","No","No","No","Internal"]
[null,null,null,10211,null,"27_28/01/2020 4:10:46 PM","2020-01-16T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Aux boiler - Both side boiler gauge glass remote operating levers in ECR deck – seized not free","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Wires were greased, eased up and now free and will be tried out regularly","2020-01-23T23:59:35","","Completed","2020-01-23T23:59:35","No","No","No","Internal"]
[null,null,null,10212,null,"27_28/01/2020 2:36:51 PM","2020-01-16T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","AE #3 - LO leakage observed on the block next to cylinder heads – Gov side","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","To check source of leakage and arrest","2020-01-18T23:59:35","","Completed","2020-01-17T23:59:35","No","No","No","Internal"]
[null,null,null,10206,null,"27_28/01/2020 5:25:41 PM","2020-01-17T23:59:35","Defect","Ship Staff","Ship Staff Insp.","ME governor actuator alarm activating at times","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Governor actuator replaced with a spare one by the Nabtesco service engineer at Singapore on 17th june20.ME tried out  and all found to be inorder.","2020-07-25T23:59:35","","Completed","2020-06-12T23:59:35","No","No","No","Internal"]
[null,null,null,10207,null,"27_28/01/2020 5:27:54 PM","2020-01-17T23:59:35","Defect","Ship Staff","Ship Staff Insp.","ME Unit no.4 Piston cooling LO.outlet temp sensor defective","E/R - Main Engine,Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Sensor renewed","2020-07-25T23:59:35","","Completed","2020-05-11T23:59:35","No","No","No","Internal"]
[null,null,null,10208,null,"27_28/01/2020 5:29:18 PM","2020-01-17T23:59:35","Defect","Ship Staff","Ship Staff Insp.","ME Unit no.3 local exh.gas temp.gauge defective","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Thermometer gauge renewed","2020-07-17T23:59:35","DLOT200051","Completed","2020-05-01T23:59:35","No","No","No","Internal"]
[null,null,null,10292,null,"27_30/01/2020 6:41:54 PM","2020-01-22T23:59:35","Defect","Ship Staff","Ship Staff Insp.","FWG Ejector pump not building up sufficient pressure and mech.seal leaking","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.31","Very High","","","Pump complete replaced with new one.","2020-02-05T23:59:35","","Completed","2020-01-23T23:59:35","No","No","No","Internal"]
[null,null,null,10493,null,"27_03/02/2020 6:19:13 PM","2020-01-27T23:59:35","Defect","Ship Staff","Ship Staff Insp.","DG1 Gov.actuator hunting/load fluctuation","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Governor actuator replaced with a new one and calibrated by the wartsila technician at Singapore on 27th Feb.2020.Presently all functions are operating satisfactory","2020-04-27T23:59:35","","Completed","2020-02-22T23:59:35","No","No","No","Internal"]
[null,null,null,10496,null,"27_09/02/2020 9:26:16 PM","2020-02-04T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Refer fish room temp sensor defective","E/R - Aux. Mach.,Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Sensor renewed","2020-02-19T23:59:35","","Completed","2020-02-05T23:59:35","No","No","No","Internal"]
[null,null,null,10494,null,"27_15/02/2020 10:25:37 AM","2020-02-06T23:59:35","Defect","Ship Staff","Ship Staff Insp.","M2 Mooring winch hyd.oil leaking from brake cylinder top part.","Deck - Mooring Machinery","Mooring","Equipment Related","9.14","Medium","","","Seals needs to be renewed, ON 17 FEB 2020 SEAL RENEWED AND LEAK RECTIFIED.","2020-05-10T23:59:35","","Completed","2020-02-12T23:59:35","No","No","No","Internal"]
[null,null,null,10495,null,"27_15/02/2020 10:29:32 AM","2020-02-07T23:59:35","Defect","Ship Staff","Ship Staff Insp.","M4 Mooring winch hyd.oil leaking from brake cylinder top part.","Deck - Mooring Machinery","Mooring","Equipment Related","9.14","Medium","","","Seal renewed","2020-05-10T23:59:35","","Completed","2020-05-03T23:59:35","No","No","No","Internal"]
[null,null,null,10646,null,"27_16/02/2020 6:17:29 PM","2020-02-10T23:59:35","Defect","Ship Staff","Ship Staff Insp.","COPT no.1 lower vibration sensor giving false alarm even in the stand still coinditions.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.8","Medium","","","Vibration  sensor cleaned and all in order.","2020-05-09T23:59:35","","Completed","2020-02-19T23:59:35","No","No","No","Internal"]
[null,null,null,11057,null,"27_11/03/2020 10:49:21 AM","2020-02-19T23:59:35","Observation","Owner / Marine / Tech. Suptd.","ISM Audit","Door packing on A-deck , CCR, Upper deck having gap. Recommanded to inspect all packing's for staircase fire doors.","Accommodation","Structural Condn. / WT integrity ","Equipment Related","5.35","Medium","","","Doors packing renewed with new ones. ","2020-08-26T23:59:35","","Completed","2020-07-05T23:59:35","No","No","No","Internal"]
[null,null,null,11058,null,"27_12/03/2020 6:54:22 AM","2020-02-19T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Cargo Audit","Drain line for stbd side no1 yellow manifold have soft patch on drain line","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","12.17","High","","","Need to rectify the fault at suitable opportunity.   - Job included in REFMAN for comming DD","2020-12-26T23:59:35","Job included in REFMAN for comming DD","Completed","2020-06-10T23:59:35","No","No","No","Internal","if this is transferred to REFFMAN, Pls close the defect - instead of keep it pending"]
[null,null,null,11059,null,"27_12/03/2020 7:15:40 AM","2020-02-19T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Cargo Audit","SAAB tank radar system giving continuous 'SCU ground failure \" alarm","Deck - Machinery","Cargo / Ballast Systems","Equipment Related","8.12","Medium","","","Need to clean the SAAB radar antenna and sensors. ETO carried out the routine and job 100% completed now.There is no alarm SCU ground failure alarm                                                                   ","2020-05-25T23:59:35","","Completed","2020-04-15T23:59:35","No","No","No","Internal"]
[null,null,null,11060,null,"27_12/03/2020 5:32:17 PM","2020-02-19T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Soft patch observed on  both port and stbd manifold drain tanks","Deck - Machinery","Cargo / Ballast Systems","Equipment Related","8.67","High","","","Need to do hot work at suitable opportunity. Job raised in REFMAN to carry out at comming drydock.","2020-12-26T23:59:35","Job raised in REFMAN to carry out at comming drydock.","Completed","2020-06-10T23:59:35","No","No","No","Internal","If included in REFFMAN, Pls close this defect in list - no need to include again in pending list"]
[null,null,null,11061,null,"27_12/03/2020 5:36:13 PM","2020-02-19T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Drain line for stbd side No-1 yellow manifold have soft patch on drain line ","Deck - Machinery","Cargo / Ballast Systems","Equipment Related","12.17","High","","","Need to do hot work at suitable opportunity. . Job raised in REFMAN to carry out at comming drydock. Duplicate job  in defect list. ","2020-12-26T23:59:35","","Completed","2020-05-23T23:59:35","No","No","No","Internal"]
[null,null,null,11062,null,"27_12/03/2020 7:04:08 AM","2020-02-19T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Cargo Audit","IG inlet valves for about 11 tanks like 4s/5s etc are not opening fully due to wasted worm gear inside.","Inert Gas","Cargo / Ballast Systems","Equipment Related","8.5","Very High","","","Need to open the valves and try to overhaul to make free.                                                             -All malfuncting pv valve worm gear overhauled on 29-feb-2020 found worm gear is in good condition after overhauling, no damage in worm gear assembly,  but v/v flap found to be very hard and unable to move completely. need to open the v/vs completely and free the flaps.         - More reqisition for complete v/v and stud nut and bolts to be raised in order to open up the v/v s to complete the job. RO RAISED.                            - Job included in REFMAN for DD as per supdt","2020-07-26T23:59:35","RO DLOT 200061 / 200103 / 200104 // - Job included in REFMAN for DD as per supdt","Completed","2020-06-10T23:59:35","No","No","No","Internal"]
[null,null,null,11067,null,"27_12/03/2020 5:27:07 PM","2020-02-19T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Channel for rubber packing wasted on No-6B & No-5 hydraulic box on deck","Deck - Machinery","Cargo / Ballast Systems","Equipment Related","11.4","Very High","","","box need to be fabricated.                                           -PRESENTLY FILLED WITH SOFT PATCH, ATTEND TO FABRICATE SOON. Covers opened up and taken to E/R workshop and fabricated. ","2020-05-26T23:59:35","","Completed","2020-04-23T23:59:35","No","No","No","Internal"]
[null,null,null,11068,null,"27_07/03/2020 4:56:44 PM","2020-02-19T23:59:35","Observation","Owner / Marine / Tech. Suptd.","ISM Audit","Emergency call button for telephone in elevator not operational and the handset was observed to be damaged.","Elect. Mach. & Equip.","Emgcy. Systems","Equipment Related","11.1","High","","","Emergency call button was verifed working and the alarm was raised on bridge on operating the button.","2020-05-18T23:59:35","","Completed","2020-02-20T23:59:35","No","No","No","Internal"]
[null,null,null,11069,null,"27_07/03/2020 4:28:18 PM","2020-02-19T23:59:35","Non Conformity","Owner / Marine / Tech. Suptd.","ISM Audit","Life buoy located  near port life boat was observed to be cracked","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.37","Low","","","Will investigate.. Life buoy renewed and placed immediately after observation. ","2020-05-18T23:59:35","","Completed","2020-02-20T23:59:35","No","No","No","Internal"]
[null,null,null,11070,null,"27_07/03/2020 4:34:19 PM","2020-02-19T23:59:35","Observation","Owner / Marine / Tech. Suptd.","ISM Audit","Few emergency lights around accomodation block not marked.","Miscellaneous","Emgcy. Systems","Equipment Related","5.18","High","","","Emg.lights needs to be marked. Lts identified and  immediately marked soon after the observation. ","2020-05-18T23:59:35","","Completed","2020-02-20T23:59:35","No","No","No","Internal"]
[null,null,null,11071,null,"27_07/03/2020 4:51:53 PM","2020-02-19T23:59:35","Observation","Owner / Marine / Tech. Suptd.","ISM Audit","Rubber gloves kept in helicopter gear not suitable for purpose as they were for chemical protection and not of insulating type for electrical protection.","Miscellaneous","Safety / LSA / FFA","Equipment Related","8.69","Medium","","","Chemical Rubber gloves to be renewed with insulates ones for electrical protection. Renewed soon after the observation.","2020-05-18T23:59:35","","Completed","2020-02-20T23:59:35","No","No","No","Internal"]
[null,null,null,11072,null,"27_07/03/2020 5:47:39 PM","2020-02-19T23:59:35","Observation","Owner / Marine / Tech. Suptd.","ISM Audit","Copy of weather and tides not available in CCR","Miscellaneous","Cargo / Ballast Systems","Inappropriate Procedure","8.7","High","","","Copy of weather and tides to be available in CCR. Weather and tide data made available in ccr during cargo operation. ","2020-05-18T23:59:35","","Completed","2020-02-19T23:59:35","No","No","No","Internal"]
[null,null,null,11073,null,"27_10/03/2020 1:30:31 PM","2020-02-19T23:59:35","Defect","Owner / Marine / Tech. Suptd.","ISM Audit","Safety guard around Fire & GS pump shaft missing","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.31","Very High","","","Guard fabricated and fitted","2020-05-18T23:59:35","","Completed","2020-03-02T23:59:35","No","No","No","Internal"]
[null,null,null,11074,null,"27_10/03/2020 1:35:47 PM","2020-02-19T23:59:35","Defect","Owner / Marine / Tech. Suptd.","ISM Audit","Pin hole in FWG ejector pump suction line","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.31","Very High","","","Leakage of blowhole on weld of the suc.pipe rectified.","2020-05-18T23:59:35","","Completed","2020-02-26T23:59:35","No","No","No","Internal"]
[null,null,null,11075,null,"27_10/03/2020 1:48:48 PM","2020-02-19T23:59:35","Defect","Owner / Marine / Tech. Suptd.","ISM Audit","Minor leakage from ME exhaust valve  no.7 unit cooling water flange","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Flange bolts tightened and no leaks now.","2020-05-18T23:59:35","","Completed","2020-02-26T23:59:35","No","No","No","Internal"]
[null,null,null,11076,null,"27_10/03/2020 3:04:43 PM","2020-02-19T23:59:35","Defect","Owner / Marine / Tech. Suptd.","ISM Audit","One(1) flange in overhead fuel line on top of the service air compressor having minor leakage.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Leaky falnge tightened","2020-05-18T23:59:35","","Completed","2020-02-29T23:59:35","No","No","No","Internal"]
[null,null,null,11077,null,"27_07/03/2020 5:54:00 PM","2020-02-19T23:59:35","Observation","Owner / Marine / Tech. Suptd.","ISM Audit","Aux.sea water pump to be used instead of main sea water pump.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.31","Very High","","","Aux.sea water pump cannot be used at sea as the main engine running demands main sea water pump.Aux.sea water pump is used in a port.","2020-05-19T23:59:35","","Completed","2020-02-20T23:59:35","No","No","No","Internal"]
[null,null,null,11078,null,"27_10/03/2020 3:15:21 PM","2020-02-19T23:59:35","Defect","Owner / Marine / Tech. Suptd.","ISM Audit","Lot of water is accumulated in the air line leading to engine room blower damper causing sluggish operation","Miscellaneous","Eng. / Strg. Comp.","Human Error","10.32","Very High","","","Engine team instructed  to drain off the water from the air bottles very frequently.","2020-05-18T23:59:35","","Completed","2020-03-05T23:59:35","No","No","No","Internal"]
[null,null,null,11079,null,"27_12/03/2020 2:19:13 PM","2020-02-19T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Most of the PV valve wire mesh have got minor holes in them","Deck - Machinery","Cargo / Ballast Systems","Equipment Related","8.41","Medium","","","renewing of wire mesh where needed                                      - All pv valve wire mesh re-inspected, and renewed as necessary, all are in intact condition now","2020-05-26T23:59:35","","Completed","2020-02-21T23:59:35","No","No","No","Internal"]
[null,null,null,11080,null,"27_12/03/2020 7:11:09 AM","2020-02-19T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Cargo Audit","one RX-517 and two GX-2009 gas meters currently not operational","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","5.23","Very High","","","As per the ship stuff Requisition already raised, need to do follow up.                                              - All required gas instruments as per req received onboard at singapore ","2020-03-26T23:59:35","","Completed","2020-02-22T23:59:35","No","No","No","Internal"]
[null,null,null,11081,null,"27_12/03/2020 2:13:21 PM","2020-02-19T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Two (2) PV valve vacuum side observed with centre washer missing","Deck - Machinery","Cargo / Ballast Systems","Equipment Related","8.41","Medium","","","centre washer need to be fitted.                                 - Center washer fabricated and fitted in place","2020-05-25T23:59:35","","Completed","2020-02-21T23:59:35","No","No","No","Internal"]
[null,null,null,11082,null,"27_10/03/2020 1:52:53 PM","2020-02-19T23:59:35","Defect","Owner / Marine / Tech. Suptd.","ISM Audit","ME unit no.6 fuel oil recirculation for fueol valve leaking from connector.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Connector tightened after applying teflon tape.","2020-05-18T23:59:35","","Completed","2020-02-27T23:59:35","No","No","No","Internal"]
[null,null,null,11083,null,"27_07/03/2020 5:57:24 PM","2020-02-19T23:59:35","Observation","Owner / Marine / Tech. Suptd.","ISM Audit","No records for performance checks of ME,Aux.engine and Boiler available onboard as the Dr.diesel equipment for taking performance not compatible in ECR computer","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","New software version v6.4b installed and performance checked for A/E1 and A/E2","2020-05-18T23:59:35","","Completed","2020-03-08T23:59:35","No","No","No","Internal"]
[null,null,null,11084,null,"27_10/03/2020 3:09:24 PM","2020-02-19T23:59:35","Defect","Owner / Marine / Tech. Suptd.","ISM Audit","Exhaust gas economiser leaking from body","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","HP Economiser leaky manhole door tightened ","2020-05-18T23:59:35","","Completed","2020-03-07T23:59:35","No","No","No","Internal"]
[null,null,null,11085,null,"27_10/03/2020 3:20:01 PM","2020-02-19T23:59:35","Defect","Owner / Marine / Tech. Suptd.","ISM Audit","Refer.room temps observed to be high","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Gas leakage checked and topped up with 5kg freon gas.","2020-05-18T23:59:35","","Completed","2020-03-08T23:59:35","No","No","No","Internal"]
[null,null,null,11086,null,"27_10/03/2020 1:44:24 PM","2020-02-19T23:59:35","Defect","Owner / Marine / Tech. Suptd.","ISM Audit","ME air cooler aft air side gasket leaking","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Refman raised to carry out repair in forthcoming DD","2020-05-18T23:59:35","Deferred to dry dock","Completed","2020-02-26T23:59:35","No","No","No","Internal"]
[null,null,null,11087,null,"27_12/03/2020 5:22:12 PM","2020-02-19T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","condition of safety chains at various elevated platform poor","Deck - Machinery","Safety / LSA / FFA","Equipment Related","11.5","Medium","","","Need to renew.                                                     -Renewed all safety chains in ig iso v/v platform, mast riser platform etc","2020-05-26T23:59:35","","Completed","2020-02-25T23:59:35","No","No","No","Internal"]
[null,null,null,11088,null,"27_12/03/2020 7:26:38 AM","2020-02-19T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","135 ltr foam Wheeled trolley fire extinguisher E-16 is suspected of leaking co2 as when the nozzle is pressed the liquid is coming out","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.42","Medium","","","Need to check all associated fittings more thoroughly and rectify the fault.                                 -ALL ASSOCIATED V/V AND HOSE ASSEMBLY CHECKED, PILOT V/V CLOSED FULLY, HOSE CHECKED NO MORE LIQUID COMMING OUT, IS IN INTACT CONDITION NOW","2020-05-19T23:59:35","","Completed","2020-03-08T23:59:35","No","No","No","Internal"]
[null,null,null,11089,null,"27_12/03/2020 7:21:26 AM","2020-02-19T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Securing belt hook for seat on aft door bent, making it difficult to operate.","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.28","Very High","","","Need to attend and rectify the fault.                         -ATTENDED AND FAULT RECTIFIED ","2020-03-26T23:59:35","","Completed","2020-03-09T23:59:35","No","No","No","Internal"]
[null,null,null,11090,null,"27_07/03/2020 5:42:32 PM","2020-02-19T23:59:35","Observation","Owner / Marine / Tech. Suptd.","ISM Audit","Junior officers are not familiar with calibration procedure for pressure and thermometer guage","Miscellaneous","Cargo / Ballast Systems","Knowledge Based","8.2","Medium","","","Junior officers to be trained in calibration of pressure and thermometer guages.                       -Training given by chief eng","2020-05-18T23:59:35","","Completed","2020-03-06T23:59:35","No","No","No","Internal"]
[null,null,null,11091,null,"27_07/03/2020 5:32:41 PM","2020-02-19T23:59:35","Observation","Owner / Marine / Tech. Suptd.","ISM Audit","Additional fire rounds in engine room and accomodation at night were not observed to be in compliance with 12.06.33.00","Miscellaneous","Safety / LSA / FFA","Behaviour Based,External Factors,Inappropriate Procedure","4.4","High","","","Fire rounds in engine room and accomodation to be in compliance with 12.06.33.00                           - PROPER FIRE PLAN MADE AND SENT OFFICE FOR APPROVAL                                                                -OFFICE APPROVAL RECEIVED                                               -PLAN EXECUTED WITH MAGNETIC CHIP PUT IN ROUND AREAS, CHECK LIST PREPARED                      ","2020-05-18T23:59:35","","Completed","2020-03-08T23:59:35","No","No","No","Internal"]
[null,null,null,11092,null,"27_07/03/2020 5:38:42 PM","2020-02-19T23:59:35","Observation","Owner / Marine / Tech. Suptd.","ISM Audit","Compass error not verified after large alterations.Additionally only sun has been used to verify compass error,other methods like transit bearings etc not used to obtain error","Navigation - Others","Navigation","Inappropriate Procedure","4.9","Medium","","","Compass error to be verified.Other methods like transit bearings to be used to obtain error.            -Compass error verified wnen ever possible once every watch, also Varified by transit bearing during transiting singapore straight","2020-05-18T23:59:35","","Completed","2020-02-25T23:59:35","No","No","No","Internal"]
[null,null,null,11093,null,"27_10/03/2020 1:40:18 PM","2020-02-19T23:59:35","Defect","Owner / Marine / Tech. Suptd.","ISM Audit","ME Jacket water cooling line One(1) flange leaking with temporarily catchment kept below it","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Leakage arrested by tightening flange bolts","2020-05-18T23:59:35","","Completed","2020-03-14T23:59:35","No","No","No","Internal"]
[null,null,null,11095,null,"27_10/03/2020 2:59:53 PM","2020-02-19T23:59:35","Defect","Owner / Marine / Tech. Suptd.","ISM Audit","ME No.3 Unit exh.temperature gauge not working","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Repeated defect,hence,closing out.","2020-05-18T23:59:35","RO DLOT200051 Applies.","Completed","2020-03-11T23:59:35","No","No","No","Internal"]
[null,null,null,11098,null,"27_12/03/2020 2:07:25 PM","2020-02-19T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Condition of safety chains at various elevated platforms poor","Deck - Machinery","Safety / LSA / FFA","Equipment Related","11.5","Medium","","","To change the safety chains.                                         - -Renewed all safety chains in ig iso v/v platform, mast riser platform etc","2020-05-26T23:59:35","","Completed","2020-02-25T23:59:35","No","No","No","Internal"]
[null,null,null,11094,null,"27_05/03/2020 11:28:52 AM","2020-02-25T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Main air compressor no.3 sol. operated drain valve passing","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Sol.operated drain valve overhauled","2020-05-08T23:59:35","","Completed","2020-02-27T23:59:35","No","No","No","Internal"]
[null,null,null,11096,null,"27_05/03/2020 11:33:10 AM","2020-02-26T23:59:35","Defect","Ship Staff","Ship Staff Insp.","AE2 Fresh water HT outlet temp higher than the normal","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Thermostatic valve renewed and all found to be inoder","2020-05-08T23:59:35","","Completed","2020-02-29T23:59:35","No","No","No","Internal"]
[null,null,null,11425,null,"27_10/04/2020 2:01:20 PM","2020-03-04T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Cargo Audit","Ship shore safety checklist point number 29 - Agreed tank venting system will be used answered as \"VESSEL DISCHARGING - MASTRISER\"","Cargo Mach.,Inert Gas","Cargo / Ballast Systems","Human Error,Inappropriate Procedure","5.9","Very High","","","To rectify in ship-shore safety c/l as \" vessel discharging\" only, striked out Mastriser and rectified fault","2020-04-25T23:59:35","","Completed","2020-04-02T23:59:35","No","No","No","Internal"]
[null,null,null,11063,null,"27_12/03/2020 9:26:03 AM","2020-03-05T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Light Post near 2C COT  weeping, rusted.","Deck - Machinery","Safety / LSA / FFA","Equipment Related","11.9","Low","","","Maintenance to schedule and carry out through chipping / painting job. Try to carry out chipping and painting job at anchor stay, with office concurrance.  Job carried out with office concurrance on 27.05.2020 at yantai anchorage","2020-05-26T23:59:35","","Completed","2020-05-22T23:59:35","No","No","No","Internal"]
[null,null,null,11064,null,"27_12/03/2020 9:34:42 AM","2020-03-05T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Light Post near 4C COT  weeping, rusted","Deck - Machinery","Safety / LSA / FFA","Equipment Related","11.9","Low","","","Thorough maintenance chipping / painting job to do. Try to carry out chipping and painting job at anchor stay, with office concurrance.","2020-05-26T23:59:35","","Completed","2020-05-30T23:59:35","No","No","No","Internal","Cant we close this job - why keep this pending for long"]
[null,null,null,11097,null,"27_12/03/2020 9:21:11 AM","2020-03-05T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Provision crane (P) operating platform safety railing missing","Deck - Machinery","Safety / LSA / FFA","Equipment Related","8.5","Very High","","","Fabricate safety railings and fit in place.                 --Railing fabricated and installed.","2020-05-26T23:59:35","","Completed","2020-03-06T23:59:35","No","No","No","Internal"]
[null,null,null,11099,null,"27_13/03/2020 10:19:30 PM","2020-03-05T23:59:35","Defect","Ship Staff","Ship Staff Insp.","ME Fuel oil booster pump no.2 motor abnormal noise","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Motor o'hauled and boxed back with new drive end bearing.Free end side bearing not renewed as having no spare","2020-06-05T23:59:35","","Completed","2020-03-06T23:59:35","No","No","No","Internal"]
[null,null,null,11100,null,"27_12/03/2020 9:49:50 AM","2020-03-05T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Mooring capstan filters and air line v/v found siezed, not operational. Also oil leakage observed from gauge glass","Deck - Mooring Machinery","Mooring","Equipment Related","9.14","Medium","","","Need to rectify the faults.                                          - SIZED AIR LINE V/V OVERHAULED, AND MADE OPERATIONAL                                                       - AIR FILTERS AND GEAR OIL FILTER CLEANED, OVERHAULED, TESED AFTER REINSTALLATION, FOUND WORKING SATISFACTORY","2020-03-26T23:59:35","","Completed","2020-03-06T23:59:35","No","No","No","Internal"]
[null,null,null,11065,null,"27_13/03/2020 10:23:13 PM","2020-03-06T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Sewage tank high level alarm float defective","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Float renewed.","2020-06-05T23:59:35","RO DLOT200076","Completed","2020-05-02T23:59:35","No","No","No","Internal"]
[null,null,null,11101,null,"27_16/03/2020 10:40:38 PM","2020-03-11T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Pump room fan no.1 coupling observed damaged","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","5.18","High","","","Coupling renewed with the spare one.","2020-06-10T23:59:35","","Completed","2020-03-12T23:59:35","No","No","No","Internal"]
[null,null,null,11102,null,"27_16/03/2020 10:42:54 PM","2020-03-11T23:59:35","Defect","Ship Staff","Ship Staff Insp.","A/Es fuel oil supply pump no.2 mech.seal passing","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Pump and motor over hauled","2020-06-10T23:59:35","","Completed","2020-03-11T23:59:35","No","No","No","Internal"]
[null,null,null,11104,null,"27_18/03/2020 1:11:21 PM","2020-03-12T23:59:35","Defect","Ship Staff","Ship Staff Insp.","A/Es fuel oil booster pump  no.2 mech seal leaking","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Pump and motor overhauled","2020-06-11T23:59:35","","Completed","2020-03-12T23:59:35","No","No","No","Internal"]
[null,null,null,11066,null,"27_01/04/2020 6:38:03 PM","2020-03-14T23:59:35","Other","Ship Staff","Ship Staff Insp.","Spares inventory update","Documentation","Cert. & Docu.","Equipment Related","10.2","Low","","","Spares inventory updated 80% in PAL PMS.Set target for completion  by ist week of June'20.","2020-06-25T23:59:35","","Completed","2020-05-26T23:59:35","No","No","No","Internal"]
[null,null,null,11103,null,"27_28/03/2020 1:41:57 PM","2020-03-17T23:59:35","Defect","Ship Staff","Ship Staff Insp.","EGB HP Circulating pump no.1 lip and mech seal passing","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Pump completely o'hauled with new bearings,lip and mech seal.","2020-06-21T23:59:35","","Completed","2020-03-22T23:59:35","No","No","No","Internal"]
[null,null,null,11105,null,"27_31/03/2020 1:41:12 PM","2020-03-17T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Refer compressor no.1 mech seal passing","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Mech.seal renewed","2020-06-16T23:59:35","","Completed","2020-03-23T23:59:35","No","No","No","Internal"]
[null,null,null,11106,null,"27_31/03/2020 1:44:00 PM","2020-03-20T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Refer compressor no.2 mech.seal leaking","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Mech.seal renewed","2020-06-19T23:59:35","","Completed","2020-03-24T23:59:35","No","No","No","Internal"]
[null,null,null,11426,null,"27_06/04/2020 3:53:15 PM","2020-03-29T23:59:35","Defect","Ship Staff","Ship Staff Insp.","EGB HP Superheater aft safety valve steam leakage from the flange gasket.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","System isolated and flange gaket renewed","2020-06-28T23:59:35","","Completed","2020-03-29T23:59:35","No","No","No","Internal"]
[null,null,null,11427,null,"27_06/04/2020 4:00:40 PM","2020-03-29T23:59:35","Defect","Ship Staff","Ship Staff Insp.","AE2 Lube oil priming pump motor making abnormal noise","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Motor overhauled and boxed back in place.","2020-06-28T23:59:35","","Completed","2020-03-29T23:59:35","No","No","No","Internal"]
[null,null,null,11428,null,"27_06/04/2020 3:57:00 PM","2020-03-30T23:59:35","Defect","Ship Staff","Ship Staff Insp.","EGB HP Superheater Fwd safety valve steam leakage from the flange gasket.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","system isolated and gasket renewed","2020-06-29T23:59:35","","Completed","2020-03-30T23:59:35","No","No","No","Internal"]
[null,null,null,11429,null,"27_06/04/2020 4:04:58 PM","2020-04-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","AE2 Priming pump mech.seal leaking","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Pump overhauled and seal renewed.","2020-06-30T23:59:35","","Completed","2020-04-02T23:59:35","No","No","No","Internal"]
[null,null,null,11430,null,"27_11/04/2020 8:21:13 PM","2020-04-02T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Cargo Audit","Ship shore checklist point no.29-Agreed tank venting system will be used answered as 'VESSEL DISCHARGING-MASTRISER","Documentation","Cert. & Docu.","Human Error","5.9","Very High","","","In the point no.29 in ship shore safety check list 'Agreed venting system'will be marked as 'Vessel Discharging'only as no venting is required during discharging.Same corrected in ship-shore safety check list.","2020-04-10T23:59:35","","Completed","2020-04-02T23:59:35","No","No","No","Internal"]
[null,null,null,11431,null,"27_11/04/2020 8:34:14 PM","2020-04-02T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Bunkering Audit","Bunker transfer plan/check list 12.04.08.011.01 section 7-monitoring of H2S/Benzene vapours:Benzene reading measured by detector tubes shall be mentioned <Min.value that can be measured by the specific tube.","Documentation","Cert. & Docu.","Human Error","10.8","Medium","","","H2S/Benzene vapour values to be checked and recorded as per the values tabulated on the gastec tube.The minimum value if obtained shall be recorded as 0/0.1 for H2S/Benzene.","2020-04-10T23:59:35","","Completed","2020-04-02T23:59:35","No","No","No","Internal"]
[null,null,null,11686,null,"27_22/04/2020 6:34:21 PM","2020-04-12T23:59:35","Defect","Ship Staff","Ship Staff Insp.","AE1 and AE2 FW preheater is not responding to the set temp.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Heater electric and water supply isolated.Fwd side end cover removed and inspected.Heater elements found clogged with dirt/mud and same cleaned up thoroughly","2020-04-25T23:59:35","","Completed","2020-04-13T23:59:35","No","No","No","Internal"]
[null,null,null,11687,null,"27_22/04/2020 6:40:01 PM","2020-04-14T23:59:35","Defect","Ship Staff","Ship Staff Insp.","AE1 and AE2 Fuel oil booster pump no.2 not building sufficient pressure","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Booster pump and regulating valve overhauled.Boxed back in place and tried out-satisfactory.","2020-06-25T23:59:35","","Completed","2020-04-16T23:59:35","No","No","No","Internal"]
[null,null,null,11866,null,"27_01/05/2020 7:28:20 PM","2020-04-18T23:59:35","Breakdown,Defect","Ship Staff","Ship Staff Insp.","While chipping on no M4 winch deck hydraulic return line, found return line cracked,  leaking and oil dipping from the crack.   ","Deck - Mooring Machinery,Deck - Pipe / Fittings","Mooring","Equipment Related","9.14","Medium","","","- Line isolated and drained, leakeage contened                                             - Line opened, removed from position                          - Blank flanges installed to stop leakage                       - new line fabricated in engine room work shop           -New line installed afterproper clean up and  pickling - Winch tested for further leakage and proper operation, found working satisfactory.","2020-04-25T23:59:35","","Completed","2020-04-20T23:59:35","No","No","No","Internal"]
[null,null,null,11683,null,"27_29/04/2020 12:54:16 PM","2020-04-23T23:59:35","Defect","Ship Staff","Ship Staff Insp.","AE2 LT inlet temp.sensor defective ","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.5","Low","","","Checked for lose connections and found to be working satisfactory","2020-07-23T23:59:35","DLOT200126","Completed","2020-08-09T23:59:35","No","No","No","Internal"]
[null,null,null,11688,null,"27_29/04/2020 1:36:13 PM","2020-04-23T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Emg.fire pump discharge line filter gasket slightly leaking","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Filter cleaned and gasket renewed.","2020-07-03T23:59:35","","Completed","2020-04-24T23:59:35","No","No","No","Internal"]
[null,null,null,11689,null,"27_29/04/2020 12:58:41 PM","2020-04-23T23:59:35","Defect","Ship Staff","Ship Staff Insp.","AE2 Limit switch|( stop lever sensor)defective","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Limit switch for stop lever sensor renewed","2020-07-23T23:59:35","","Completed","2020-04-24T23:59:35","No","No","No","Internal"]
[null,null,null,11684,null,"27_29/04/2020 4:30:41 PM","2020-04-24T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Main engine Diesel doctor performance moniitor crank angle optical sensor defective","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.21","Medium","","","Optical sensors recd .at Singapore on 16th June 2020 and same day replaced.Performance taken on 25th june20 and all found to be in order.","2020-07-24T23:59:35","RO raised for the spare connector. ","Completed","2020-06-20T23:59:35","No","No","No","Internal"]
[null,null,null,11685,null,"27_29/04/2020 4:39:20 PM","2020-04-24T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Cargo tank no.1port and 4 centre IG pressure sensor giving wrong reading","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.23","Medium","","","Sensors renewed","2020-07-23T23:59:35","","Completed","2020-05-02T23:59:35","No","No","No","Internal"]
[null,null,null,19415,null,"27_06/05/2021 1:21:13 PM","2020-04-25T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Remote gauge/vlave relasing levers in ECR platform found seized, not connected properly","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Remote easing gears eased up","2021-05-15T23:59:35","","Completed","2021-05-05T23:59:35","No","No","No","Internal"]
[null,null,null,11867,null,"27_06/05/2020 1:15:48 PM","2020-04-29T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Ejector pump delivery valve passing","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Valve overhauled.","2020-07-30T23:59:35","","Completed","2020-04-30T23:59:35","No","No","No","Internal"]
[null,null,null,11868,null,"27_06/05/2020 1:19:45 PM","2020-04-30T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Ejector pump suction pipe after the filter corroded/holed.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Pipe 1200mm L x 100mm NB with one 90degree fabricated","2020-07-30T23:59:35","","Completed","2020-04-30T23:59:35","No","No","No","Internal"]
[null,null,null,11864,null,"27_06/05/2020 1:23:26 PM","2020-05-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","AE3 fuel oil booster pump standby mode pressure switch defective","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.2","Low","","","Replaced with spare pressure switch received and now its working fine. ","2020-08-25T23:59:35","","Completed","2020-08-19T23:59:35","No","No","No","Internal"]
[null,null,null,11865,null,"27_12/05/2020 8:32:18 AM","2020-05-02T23:59:35","Defect","Ship Staff","Ship Staff Insp.","MSW Pump no.2 discharge valve leaking from the body.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.1","Medium","","","Valve renewed with a spare one.","2020-08-02T23:59:35","","Completed","2020-06-24T23:59:35","No","No","No","Internal"]
[null,null,null,11869,null,"27_12/05/2020 8:34:58 AM","2020-05-04T23:59:35","Defect","Ship Staff","Ship Staff Insp.","LT Cooler no.1 sea water outlet valve leaking from the body.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Valve replaced with the new one.","2020-08-04T23:59:35","","Completed","2020-05-10T23:59:35","No","No","No","Internal"]
[null,null,null,11970,null,"27_19/05/2020 5:43:49 AM","2020-05-14T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Port side pump room fan \"BHD STUFF BOX TEMP\" not readable.  Temp controller unit malfunctioing.","Elect. Mach. & Equip.","Cargo / Ballast Systems","Equipment Related","5.18","High","","","Sensor replaced and observed to be functioning  properly","2020-08-14T23:59:35","","Completed","2020-06-13T23:59:35","No","No","No","Internal"]
[null,null,null,11971,null,"27_19/05/2020 6:00:25 AM","2020-05-14T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Minor drop drop hydraulic oil leakage from valve hydraulic room pipe stak where all hydraulic lines penetrating the fwd bulkhead. Unable to identify the leaking line / coupling. ","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","6.4","High","","","Defect also raised previously and closed. Again leakage started as position of  leakage could not be identified because of all line coinciding in one place. Work in progress. Same raised in Refman for coming DD","2020-08-14T23:59:35","Job raised in REFMAN for coming DD","Completed","2020-06-10T23:59:35","No","No","No","Internal"]
[null,null,null,11972,null,"27_28/05/2020 2:18:11 PM","2020-05-15T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Harbour sea water pump mech.seal passing","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.1","Medium","","","Mech.seal and shaft sleeve renewed.","2020-08-15T23:59:35","","Completed","2020-05-24T23:59:35","No","No","No","Internal"]
[null,null,null,11973,null,"27_28/05/2020 2:26:16 PM","2020-05-17T23:59:35","Guarantee Claim","Ship Staff","Ship Staff Insp.","EGCS Sea water no.1 to be opened up for inspection of the pump casing and impeller.","E/R - Pumps","Eng. / Strg. Comp.","Behaviour Based","10.31","Very High","","","Pump dimantled ,inspected and all found to be in order.","2020-08-16T23:59:35","","Completed","2020-05-17T23:59:35","No","No","No","Internal"]
[null,null,null,16661,null,"27_04/01/2021 7:40:59 PM","2020-05-31T23:59:35","Observation","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","ONE OF THE ENGINE ROOM PORTABLE RADIO ANTENNA FOUND DAMAGED, WHICH WAS COVERED WITH AN INSULATION TAPE.","Miscellaneous","Crew Management","Behaviour Based","4.26","Low","","","NEW ANTENNA REPLACED.","2020-08-26T23:59:35","","Completed","2020-06-12T23:59:35","No","No","No","External"]
[null,null,null,17752,null,"27_Wed Feb 10 2021 09:42:03 GMT+0000","2020-05-31T23:59:35","Observation","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","One portable radio provided in engine control room was found with antenna crack broken and temporarily repaired with electrical insulation tape.","Navigation - Others","Navigation","Equipment Related","4.26","Low","","","The antenna with the cracked sheathing was disconnected from the portable radio and discarded and a new antenna from on board spares was installed on the portable radio.","2020-06-15T23:59:35","","Completed","2020-05-31T23:59:35","No","No","No","External"]
[null,null,null,12895,null,"27_15/06/2020 11:27:30 AM","2020-06-08T23:59:35","Defect","Ship Staff","Ship Staff Insp.","AE3 F.O.Unit,F.O.Booster pump no.1 and 2mech.seal leaking","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.2","Low","","","Seal leakage is the minimum which is less than 10 drops per hour and that much is required for the lubrication of the contact faces to prevent failure as per the instruction manual of FCU.","2020-09-07T23:59:35","GC raised and will receive onboard soon..","Completed","2020-08-23T23:59:35","No","No","No","Internal"]
[null,null,null,12908,null,"27_19/06/2020 9:10:44 AM","2020-06-11T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Lube oil purifier temp regulating valve malfunctioning","E/R - Purifier","Eng. / Strg. Comp.","Equipment Related","10.2","Low","","","Temp regulating valve renewed. and responding satisfactory","2020-06-11T23:59:35","Spare temp. reg.valve recd on 16th June20 at Singapore","Completed","2020-06-14T23:59:35","No","No","No","Internal"]
[null,null,null,12909,null,"27_19/06/2020 9:14:09 AM","2020-06-11T23:59:35","Defect","Ship Staff","Ship Staff Insp.","HFO Purifier temp .regulating valve inoperative","E/R - Purifier","Eng. / Strg. Comp.","Equipment Related","10.2","Low","","","Temp.reg.valve renewed and functioning satisfactory.","2020-09-11T23:59:35","Spare temp.reg.valve recd.at Singapore on 16th June 20","Completed","2020-06-15T23:59:35","No","No","No","Internal"]
[null,null,null,12894,null,"27_26/06/2020 10:45:28 AM","2020-06-12T23:59:35","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Main deck pipe stacks -Pipe under supports are under various stage of corrosion-on sec.fwd of the manifold.","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.4","Very High","","","Hydroblasting and painting of main deck pipe stacks & supports in fwd near 1C area completed  in ballast passage. Stopped due to sprays (laden passage). Will contiue the job in ballast passage again","2020-12-12T23:59:35","","Completed","2020-08-28T23:59:35","No","No","No","Internal","As this is an ongoing long time maintenance plan, target date for completion  shall be kept realistic till Dec 2020.\nRegular updates are being rec'd regularly vide weekly updates"]
[null,null,null,12896,null,"27_25/06/2020 10:37:10 PM","2020-06-12T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Oil leaks found in the pipe bunch existing from VRCS room.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","10.32","Very High","","","To check exact/pipe by isolating the valve sections and identify the leaking pipe. All hydraulic couplings were rechecked for tighteness in hyd room.  NO leaks had been observed in the hydraulic in last loading or discharging operation","2020-09-12T23:59:35","","Completed","2020-09-11T23:59:35","No","No","No","Internal"]
[null,null,null,12897,null,"27_25/06/2020 10:42:31 PM","2020-06-12T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Fire damper control flap for upper deck-Postion shows CLOSE but switch shows in TEST","Accommodation","Eng. / Strg. Comp.","Equipment Related","5.34","Low","","","The switch position on B/R c/o and now it shows the right position","2020-06-28T23:59:35","","Completed","2020-06-27T23:59:35","No","No","No","Internal"]
[null,null,null,12898,null,"27_26/06/2020 10:20:25 AM","2020-06-12T23:59:35","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Life boat Battery isolator not yet fitted","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.29","High","","","Emergency generator and both life boats  battery isolator installed and batteries renewed.","2020-06-28T23:59:35","","Completed","2020-07-02T23:59:35","No","No","No","Internal"]
[null,null,null,12899,null,"27_26/06/2020 10:37:47 AM","2020-06-12T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Emergency generator exhausts pipe spark arrestor missing","Deck - Pipe / Fittings","Emgcy. Systems","Equipment Related","10.32","Very High","","","Spark arrester with flange joint arrangement  fabricated and put in place.","2020-06-28T23:59:35","","Completed","2020-07-13T23:59:35","No","No","No","Internal"]
[null,null,null,12900,null,"27_26/06/2020 10:57:13 AM","2020-06-12T23:59:35","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Tank top near Stbd side sea chest filter-rust spots","Miscellaneous","Cargo / Ballast Systems","Equipment Related","10.32","Very High","","","Area chipped ,primer applied and painted.","2020-07-12T23:59:35","","Completed","2020-07-06T23:59:35","No","No","No","Internal"]
[null,null,null,12910,null,"27_26/06/2020 10:49:04 AM","2020-06-12T23:59:35","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","EGB Casing and adjac areas behind the HP coil section platform-bulkheads/floors/pipe dirty","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","11.4","Very High","","","Clean up and painted as required.","2020-07-12T23:59:35","","Completed","2020-06-20T23:59:35","No","No","No","Internal"]
[null,null,null,12911,null,"27_26/06/2020 10:52:20 AM","2020-06-12T23:59:35","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Funnel casing lots of soot/dirt on upper funnel casing decks","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Funnel casing area mopped/cleaned and painted as required.","2020-07-12T23:59:35","","Completed","2020-06-20T23:59:35","No","No","No","Internal"]
[null,null,null,12912,null,"27_26/06/2020 11:01:37 AM","2020-06-12T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Pump room blower bearing temp sensor observed to be in alarm condition","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","5.18","High","","","Sensor renewed and calibrated-all in order","2020-06-20T23:59:35","","Completed","2020-06-14T23:59:35","No","No","No","Internal"]
[null,null,null,12913,null,"27_26/06/2020 10:05:39 AM","2020-06-12T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Old bunch of safety harness found lying in deck stores","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.5","Low","","","All old safety harness discarded and put in garbage.","2020-06-20T23:59:35","","Completed","2020-06-19T23:59:35","No","No","No","Internal"]
[null,null,null,12914,null,"27_26/06/2020 10:26:46 AM","2020-06-12T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Stern light post base frame rusted","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.1","High","","","Derusting and painting of the Stern post completed","2020-06-28T23:59:35","","Completed","2020-06-21T23:59:35","No","No","No","Internal"]
[null,null,null,12915,null,"27_26/06/2020 10:34:40 AM","2020-06-12T23:59:35","Critical Equipment","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Portable fire extinguishers Accom/Deck/EGCS-June check does not found in the tag","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.4","High","","","All fire extinguishers rechecked. Dates verified.","2020-06-20T23:59:35","","Completed","2020-06-20T23:59:35","No","No","No","Internal"]
[null,null,null,12916,null,"27_26/06/2020 10:40:54 AM","2020-06-12T23:59:35","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Side Navigation lights base being corroded","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.1","High","","","Derusting and painting of side lights post and adjacent areas completed.","2020-07-12T23:59:35","","Completed","2020-06-21T23:59:35","No","No","No","Internal"]
[null,null,null,12917,null,"27_26/06/2020 10:14:35 AM","2020-06-12T23:59:35","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","AHU room Mech.vent fan was kept running in the AHU room,which was drawing all cold air and venting to China passage","Accommodation","Eng. / Strg. Comp.","Equipment Related","5.45","Medium","","","Mech.exhaust vent fan stopped and the Natural ventilation door flap kept open.","2020-06-20T23:59:35","","Completed","2020-06-20T23:59:35","No","No","No","Internal"]
[null,null,null,12918,null,"27_26/06/2020 9:58:21 AM","2020-06-12T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Low expansion foam room 1 no.bulb found fused","Critical Equip.","Safety / LSA / FFA","Equipment Related","11.1","High","","","Fused Bulb Replaced","2020-06-20T23:59:35","","Completed","2020-06-20T23:59:35","No","No","No","Internal"]
[null,null,null,12919,null,"27_26/06/2020 11:06:44 AM","2020-06-12T23:59:35","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","AE2 Oil max filter found not running","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Discussed with the engine team to ensure oil max filter to be kept running always.","2020-06-20T23:59:35","","Completed","2020-06-20T23:59:35","No","No","No","Internal"]
[null,null,null,12920,null,"27_26/06/2020 11:04:11 AM","2020-06-12T23:59:35","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","AE1 Oil max filter found not running","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Discussed with the engine team to ensure oil max filter to be kept running always.","2020-06-20T23:59:35","","Completed","2020-06-20T23:59:35","No","No","No","Internal"]
[null,null,null,12921,null,"27_26/06/2020 10:30:10 AM","2020-06-12T23:59:35","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","EGCS Ventilation flaps operation-open/close periodic checks","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","5.45","Medium","","","CRF Raised and office approved on 29th June20","2020-06-28T23:59:35","","Completed","2020-06-24T23:59:35","No","No","No","Internal"]
[null,null,null,12922,null,"27_26/06/2020 10:01:48 AM","2020-06-12T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Fire control station entry door from accomodation side very tight to open and close,not free in the frames","Accommodation","Safety / LSA / FFA","Equipment Related","5.34","Low","","","Fire door operation eased and made free.","2020-06-28T23:59:35","","Completed","2020-06-21T23:59:35","No","No","No","Internal"]
[null,null,null,12904,null,"27_19/06/2020 9:19:55 AM","2020-06-13T23:59:35","Defect","Ship Staff","Ship Staff Insp.","E/R Workshop A/C unit ckt breaker tripping on overload.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","A/C Compressor replaced with a spare one.Gas charged to the system and observed to be working satisfactory.","2020-09-13T23:59:35","","Completed","2020-08-09T23:59:35","No","No","No","Internal"]
[null,null,null,13162,null,"27_11/07/2020 2:50:08 PM","2020-06-14T23:59:35","Defect","Ship Staff","Ship Staff Insp.","EGCS CEMS shows failure alarm and emission data readings are not available","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.11","Medium","","","Carried out as advised by the Makers HGS and CEMS giving the values now.","2020-09-14T23:59:35","","Completed","2020-08-05T23:59:35","No","No","No","Internal"]
[null,null,null,12905,null,"27_24/06/2020 4:29:14 PM","2020-06-15T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Bridge CCTV Port side camera defective","Navigation - DGPS / EPFS / AIS","Navigation","Equipment Related","11.1","High","","","Camera replaced with a spare one and found to operating satisfactory.","2020-09-15T23:59:35","RO DLOT200129 applies.","Completed","2020-08-11T23:59:35","No","No","No","Internal"]
[null,null,null,12923,null,"27_22/06/2020 11:37:01 AM","2020-06-15T23:59:35","Defect","Ship Staff","Ship Staff Insp.","AE3 F.O.Temterature controller and sensor erratic","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Found the connection loose which was tightened. System back to normal ","2020-09-15T23:59:35","Office informed and GC raised.","Completed","2020-06-22T23:59:35","No","No","No","Internal"]
[null,null,null,12925,null,"27_25/06/2020 10:31:49 PM","2020-06-15T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Refer comp.performance deterioated and comp.shaft worn out IWO shaft seal","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Refer compressor renewed with a spare one.","2020-09-15T23:59:35","","Completed","2020-06-20T23:59:35","No","No","No","Internal"]
[null,null,null,12924,null,"27_29/06/2020 6:58:05 PM","2020-06-20T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Bridge AC (Port Side) is not working","Accommodation","MLC Related","Equipment Related","11.1","High","","","Found Compressor capacitor terminals burnt. Same was rectified. Now operational","2020-06-25T23:59:35","","Completed","2020-06-24T23:59:35","No","No","No","Internal"]
[null,null,null,12907,null,"27_30/06/2020 9:44:51 PM","2020-06-25T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Midship hose handling Port Crane Cam Limit switch malfunctioning ","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.5","Very High","","","Cam limit switch replaced with spare new one. Operation checked and all found to be in order. ","2020-09-25T23:59:35","RO DLOT200186 applies","Completed","2020-08-08T23:59:35","No","No","No","Internal"]
[null,null,null,13250,null,"27_25/07/2020 8:13:06 PM","2020-07-20T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Aux.boilers monitor observed not responding","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Monitor replaced with a good old one which is working satisfactory.","2020-10-20T23:59:35","","Completed","2020-07-28T23:59:35","No","No","No","Internal"]
[null,null,null,13249,null,"27_01/08/2020 7:09:48 PM","2020-07-21T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Master sream valve for the Mast riser and port slop tank heating coils observed leaking","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","8.24","Medium","","","Valve replaced with a spare one.","2020-08-27T23:59:35","","Completed","2020-07-27T23:59:35","No","No","No","Internal"]
[null,null,null,13248,null,"27_01/08/2020 7:13:39 PM","2020-07-25T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Deck seal steam heating coil inlet and return valve found to be passing","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.35","Medium","","","Valves repalced with the old good ones.","2020-08-25T23:59:35","","Completed","2020-07-28T23:59:35","No","No","No","Internal"]
[null,null,null,13435,null,"27_08/08/2020 7:19:55 PM","2020-07-28T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Aux.boiler no.1 Auto feed water valve not responding to the water level demand ","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Auto feed valve diaphragm renewed.Valve operation checked and observed to be working satisfactory.","2020-10-28T23:59:35","RO DLOT200208 raised","Completed","2020-10-10T23:59:35","No","No","No","Internal"]
[null,null,null,13437,null,"27_08/08/2020 7:23:53 PM","2020-07-28T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Aux.engine no.1 flywheel rim teeth damaged","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Flywheel rim renewed","2020-08-28T23:59:35","","Completed","2020-08-01T23:59:35","No","No","No","Internal"]
[null,null,null,13438,null,"27_13/08/2020 2:38:05 PM","2020-07-29T23:59:35","Defect","Ship Staff","Ship Staff Insp.","OWS motor driven oil valve inoperational ","Critical Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Valve replaced with a spare one. ","2020-10-28T23:59:35","RO Raised","Completed","2020-08-10T23:59:35","No","No","No","Internal"]
[null,null,null,13643,null,"27_25/08/2020 1:42:18 AM","2020-08-08T23:59:35","Defect","Ship Staff","Ship Staff Insp.","STBD Hose handling crane hoisting limit switch malfunctioning","Deck - Machinery","Cargo / Ballast Systems","Equipment Related","8.5","Very High","","","Hoisting limit switch adjusted and now its working fine","2020-08-25T23:59:35","","Completed","2020-08-19T23:59:35","No","No","No","Internal"]
[null,null,null,13436,null,"27_15/08/2020 9:20:25 AM","2020-08-08T23:59:35","Defect","Ship Staff","Ship Staff Insp.","AE1 & AE2 Viscotherm steam control valve erratic","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Actuator drive damaged gear assy repaired and found all in order.","2020-11-08T23:59:35","DLOT200140 Raised","Completed","2020-09-20T23:59:35","No","No","No","Internal"]
[null,null,null,13439,null,"27_15/08/2020 9:26:55 AM","2020-08-09T23:59:35","Defect","Ship Staff","Ship Staff Insp.","AE2 MCM-11Board for safeties found to be malfunctioning","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","MCM-11 Board replaced with a spare one. ","2020-11-09T23:59:35","","Completed","2020-08-09T23:59:35","No","No","No","Internal"]
[null,null,null,13641,null,"27_18/08/2020 6:18:08 AM","2020-08-11T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Main air compressor No.1 parameter monitoring PLC defective","E/R - Air Comp.","Eng. / Strg. Comp.","External Factors","10.32","Very High","","","PLC renewed and compressor observed to performing well.","2020-11-11T23:59:35","RO DLOT200220 raised.","Completed","2020-10-10T23:59:35","No","No","No","Internal"]
[null,null,null,13642,null,"27_25/08/2020 4:28:19 PM","2020-08-11T23:59:35","Breakdown,Defect","Ship Staff","Ship Staff Insp.","CCR wind observator is not function. On startup the screen it shows “failed to open! OMD data online” error message.\t\t\t\t ","Miscellaneous","Cargo / Ballast Systems","Equipment Related","","","","","Software issue. Rectified by makers by taking remote access of the system. System is working fine now.","2020-10-11T23:59:35","","Completed","2020-09-30T23:59:35","No","No","No","Internal"]
[null,null,null,13644,null,"27_18/08/2020 6:10:40 AM","2020-08-11T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Port and Stb lifeboat winch brake handle limit switch malfunctioning.","Critical Equip.","Safety / LSA / FFA","Equipment Related","10.3","Medium","","","Limit switches renewed and operation tested-Working satisfactory.","2020-11-10T23:59:35","","Completed","2020-08-20T23:59:35","No","No","No","Internal"]
[null,null,null,13645,null,"27_18/08/2020 6:14:25 AM","2020-08-12T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Main air compressor No.2 auto unloader solenoid operated drain valve passing","E/R - Air Comp.","Eng. / Strg. Comp.","External Factors","10.32","Very High","","","Replaced with spare solenoid valve received. ","2020-11-11T23:59:35","","Completed","2020-08-17T23:59:35","No","No","No","Internal"]
[null,null,null,12901,null,"27_01/07/2020 23:16:39","2020-08-17T23:59:35","Observation","Ship Staff","Ship Staff Insp.","1.\tRADAR OVERLAY FROM X & S BAND RADAR HAS STOPPED WORKING ON BOTH ECDIS AFTER INSTALLION OF NEW X BAND RADAR & SAME WAS BOUGHT INTO NOTICE OF TECHNICIANS PRIOR DEPARTURE.\n\n\n\n2.\tARPA TARGETS MISSING FROM NEWLY FITTED X BAND RADAR ON BOTH ECDIS.\n\n\n\n3.\tObserved when S band RADAR is switched off, the X band RADAR goes to standby mode automatically after Error ''TX/RX communication error- There is a communication error with RADAR antenna'' appears on the X band radar screen\n\n\n\n","Navigation - RADAR","Navigation","Equipment Related","4.17","Very High","","","\n\n\n\n\n\n\n\n1.\tREMOTELY ACCESS TAKEN BY MAKERS TECHNICIAN, BUT IT COULD NOT RESOLVE THE ISSUE\n\n\n\n2.\tCOMMUNICATION IN PROGRESS WITH MAKERS TECHNICIANS & ADVISED TO ADD INTERSWITCH TO RADAR AT NEXT PORT CALL SINGAPORE. REMOTELY CHECKED BY MAKERS TECHNICIAN, BUT IT COULD NOT RESOLVE THE ISSUE\n\n\n\nSERVICING DONE DURING DD AT YULIAN AND OVERLAY FROM BOTH RADAR CAN BE SEEN ON ECDIS.\n\n\n\n","2020-12-25T23:59:35","","Completed","2020-11-23T23:59:35","No","No","No","Internal"]
[null,null,null,12903,null,"27_01/07/2020 23:31:09","2020-08-18T23:59:35","Observation","Ship Staff","Ship Staff Insp.","AIS Target found to be missing during playback on both ECDIS ","Navigation - ECDIS","Navigation","Equipment Related","4.17","Very High","","","EMAIL CONFIRMATION RECEIVED FROM MAKER STATING THAT AIS/ARPA TARGETS ARE DISPLAYED IN THE LOGBOOK","2020-12-25T23:59:35","","Completed","2020-10-08T23:59:35","No","No","No","Internal"]
[null,null,null,12902,null,"27_01/07/2020 23:26:18","2020-08-20T23:59:35","Observation","Ship Staff","Ship Staff Insp.","ARPA TARGETS MISSING FROM NEWLY FITTED X BAND RADAR ON BOTH ECDIS.","Navigation - DGPS / EPFS / AIS","Navigation","Equipment Related","4.17","Very High","","","job reassigned under new defect","2020-11-25T23:59:35","","Completed","2020-09-25T23:59:35","No","No","No","Internal"]
[null,null,null,13646,null,"27_30/08/2020 5:41:55 PM","2020-08-22T23:59:35","Defect","Ship Staff","Ship Staff Insp.","ME Unit No.7 Exhaust gas temperature local thermometer defective. ","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Replaced with spare one. Now its showing proper reading. ","2020-08-25T23:59:35","","Completed","2020-08-23T23:59:35","No","No","No","Internal"]
[null,null,null,13947,null,"27_14/09/2020 9:12:53 PM","2020-09-03T23:59:35","Defect","Ship Staff","Ship Staff Insp.","HFO Purifier no.1 feed pump mechanical seal leaking","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Seal renewed","2020-12-02T23:59:35","","Completed","2020-09-06T23:59:35","No","No","No","Internal"]
[null,null,null,13948,null,"27_14/09/2020 9:16:33 PM","2020-09-04T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Main engine fuel oil booster pump no.2 mech seal leaking","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Seal renewed.","2020-11-03T23:59:35","","Completed","2020-09-09T23:59:35","No","No","No","Internal"]
[null,null,null,14107,null,"27_30/09/2020 9:33:01 AM","2020-09-11T23:59:35","Defect","Ship Staff","Ship Staff Insp.","AE1& AE2 Fuel oil booster pump no.2 mech.seal passing","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Seal renewed","2020-09-25T23:59:35","","Completed","2020-09-11T23:59:35","No","No","No","Internal"]
[null,null,null,14108,null,"27_30/09/2020 9:36:32 AM","2020-09-12T23:59:35","Defect","Ship Staff","Ship Staff Insp.","AE2 L.O.Priming pump mech seal leaking","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Seal renewed","2020-10-11T23:59:35","","Completed","2020-09-12T23:59:35","No","No","No","Internal"]
[null,null,null,14109,null,"27_30/09/2020 9:40:10 AM","2020-09-13T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Vac Condenser sea water circ.pump mech seal leaking","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Pump dismantled and boxed back with new seal,shaft sleeve and gaskets","2020-12-12T23:59:35","","Completed","2020-09-15T23:59:35","No","No","No","Internal"]
[null,null,null,14105,null,"27_29/09/2020 9:36:37 PM","2020-09-20T23:59:35","Observation","Ship Staff","Ship Staff Insp.","VDR system lost feed from X band radar, so extracted file do not show radar image in live software player (Error Code- 42) and during VDR Playback, Latitude and Longitude values are also partially missing.","Navigation - VDR / BNWAS","Navigation","Equipment Related","4.7","High","","","Error issue of 042 code rectified after troubleshooting.","2020-12-20T23:59:35","","Completed","2020-10-05T23:59:35","No","No","No","Internal"]
[null,null,null,14106,null,"27_29/09/2020 9:40:33 PM","2020-09-21T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Observed when S band RADAR is switched off, the X band RADAR goes to standby mode automatically after Error ''TX/RX communication error- There is a communication error with RADAR antenna'' appears on the X band radar screen","Navigation - RADAR","Navigation","Equipment Related","","","","","job reassigned under new defect","2020-12-20T23:59:35","","Completed","2020-09-25T23:59:35","No","No","No","Internal"]
[null,null,null,14277,null,"27_04/10/2020 5:32:28 AM","2020-09-27T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Main engine unit no.7 fuel oil HP pipe minute leakage from the union ","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Union renewed and there is no leak detected.","2021-03-26T23:59:35","","Completed","2020-12-27T23:59:35","No","No","No","Internal"]
[null,null,null,14279,null,"27_09/10/2020 3:56:29 PM","2020-09-28T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Aux.boiler no.2 Fuel oil electric actuator malfunctioning","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.2","Low","","","Actuator renewed by replacing ES11 from the defective actuator which was missing in the new actuator.","2020-12-25T23:59:35","RO DLOT200226","Completed","2020-10-10T23:59:35","No","No","No","Internal"]
[null,null,null,14278,null,"27_13/10/2020 5:06:35 PM","2020-09-30T23:59:35","Defect","Ship Staff","Ship Staff Insp.","HP Circ.pump no.1 not building sufficient pressure","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Replaced the magnectic couplings (inner and outer) ","2020-12-25T23:59:35","","Completed","2020-10-14T23:59:35","No","No","No","Internal"]
[null,null,null,14280,null,"27_09/10/2020 3:52:41 PM","2020-10-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","LT.Cooler no.2 filter cover corroded /pin holed.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.2","Low","","","Cooler isolated and fiter cover renewed with the fabricated one.","2020-12-21T23:59:35","RO200195","Completed","2020-10-01T23:59:35","No","No","No","Internal"]
[null,null,null,22357,null,"27_30/10/2021 1:13:43 PM","2020-10-14T23:59:35","Defect","Ship Staff","Ship Staff Insp.","MSW Pump no.1 suction valve body corroded/wasted.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Valve needs to be renewed.","2022-01-13T23:59:35","","Completed","2020-11-15T23:59:35","No","No","No","Internal"]
[null,null,null,14396,null,"27_24/10/2020 10:28:38 AM","2020-10-15T23:59:35","Defect","Ship Staff","Ship Staff Insp.","EGCS CEMS failure alarm triggered. ","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.3","Medium","","","Cleaned the Sampling gas proble filter and cell analyser inlet filter. Alarm got reset and system back to normal. ","2020-10-25T23:59:35","","Completed","2020-10-15T23:59:35","No","No","No","Internal"]
[null,null,null,14397,null,"27_24/10/2020 10:25:09 AM","2020-10-16T23:59:35","Defect","Ship Staff","Ship Staff Insp.","EGCS WMS002 low flow alarm triggered","E/R - Pumps,Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.3","Medium","","","Pump replaced with spare one. ","2020-10-25T23:59:35","","Completed","2020-10-16T23:59:35","No","No","No","Internal"]
[null,null,null,14394,null,"27_30/10/2020 3:52:42 PM","2020-10-19T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","1P COT Pressure sensor is inoperational, showing reading of about 2400 mmwg eventhought the tank pressure was about 400 mmWg\t\t","Inert Gas","Cargo / Ballast Systems","Equipment Related","8.19","High","","","PRESSURE SENSOR REPLACED AND RECTIFIED.","2020-12-26T23:59:35","DLOT200309 RECEIVED DURING DD","Completed","2020-12-01T23:59:35","No","No","No","Internal"]
[null,null,null,14395,null,"27_31/10/2020 9:44:04 AM","2020-10-22T23:59:35","Defect","Ship Staff","Ship Staff Insp.","LT Cooler NO.2 sea water side reducer weld seam leaking ","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.3","Medium","","","Reducer replaced by the dockyard and no leaks now. ","2020-12-25T23:59:35","","Completed","2020-12-03T23:59:35","No","No","No","Internal"]
[null,null,null,14638,null,"27_13/11/2020 8:35:30 AM","2020-11-03T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Main engine cylinder liner temp monitoring system failure","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.3","Medium","","","Monitor and PC old one programmed by the Wartsila service engineer and now dispalying the liner wall temp.","2020-12-25T23:59:35","DLOT200317 Applies","Completed","2020-12-10T23:59:35","No","No","No","Internal"]
[null,null,null,14637,null,"27_13/11/2020 8:41:21 AM","2020-11-05T23:59:35","Defect","Ship Staff","Ship Staff Insp.","W/H Defrost heater inoperational which is showing zero insulation resistance","Navigation - Others","Navigation","Equipment Related","10.32","Very High","","","Heater elements renewed","2020-12-25T23:59:35","DLOT 200324 Applies","Completed","2020-12-10T23:59:35","No","No","No","Internal"]
[null,null,null,14639,null,"27_13/11/2020 8:55:25 AM","2020-11-05T23:59:35","Defect","Ship Staff","Ship Staff Insp.","AE1 unit no.4,5 and 6 showing higher temp as compared to other units.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Fuel valves pressure tested and tappet clearances checked-still no change.T/C Cartridge removed from place and observed nozzle ring in line with the exhaust manifold  of these units partially clogged.T/C parts cleaned and boxed back-alll in order","2020-12-25T23:59:35","DLOT200317 Applies","Completed","2020-11-07T23:59:35","No","No","No","Internal"]
[null,null,null,15737,null,"27_23/11/2020 3:22:25 PM","2020-11-11T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Main air compressor no.2 and 3 start panel PLC failure due to aging.","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","PLC  renewed. WORKING SATISFACTORY","2021-02-22T23:59:35","","Completed","2021-01-12T23:59:35","No","No","No","Internal"]
[null,null,null,16653,null,"27_24/12/2020 8:32:40 AM","2020-12-11T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Unit No 2 and 5, minor water leakage from the blanked lubricating quills","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.3","Medium","","","O RINGS RENEWED. NOW NO MORE LEAK IN THE SYSTEM ","2021-03-11T23:59:35","","Completed","2020-12-27T23:59:35","No","No","No","Internal"]
[null,null,null,17433,null,"27_16/01/2021 9:25:11 PM","2020-12-18T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Engine Room bottom floor plate near EGCS to secure","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","11.4","Very High","","","BOTTOM PLATFORM ALL BOLTS SECURED","2021-03-17T23:59:35","","Completed","2021-02-20T23:59:35","No","No","No","Internal"]
[null,null,null,17434,null,"27_16/01/2021 10:04:42 PM","2020-12-18T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","FUNNEL FLAP S AIR SUPPLY NOT SECURED.\t","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","5.19","Medium","","","AIR SUPPLY LINE SECURED","2021-01-29T23:59:35","","Completed","2021-02-06T23:59:35","No","No","No","Internal"]
[null,null,null,17435,null,"27_17/01/2021 4:44:04 PM","2020-12-18T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ME AIR COOLER (FWD) SLIGHT WATER LEAKAGE AROUND THE FEW LN BOLTS","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.19","Very High","","","LEAK TO BE RECTIFIED.","2021-01-28T23:59:35","","Completed","2020-12-29T23:59:35","No","No","No","Internal"]
[null,null,null,17436,null,"27_17/01/2021 4:45:25 PM","2020-12-18T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ME RPLS SYSTEM SLIGHT OIL LEAKAGE","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.19","Very High","","","LEAK TO BE RECTIFIED.","2021-01-27T23:59:35","","Completed","2020-12-29T23:59:35","No","No","No","Internal"]
[null,null,null,17437,null,"27_17/01/2021 4:47:57 PM","2020-12-18T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ME AFT SIDE OIL LEAKAGE AT EMERGENCY MANO DECK","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.19","Very High","","","LEAK RECTIFIED.","2021-02-03T23:59:35","","Completed","2021-01-20T23:59:35","No","No","No","Internal"]
[null,null,null,17447,null,"27_16/01/2021 8:55:33 PM","2020-12-18T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","em generator room fire sensor alam push button fallen loose","Elect. Mach. & Equip.","Emgcy. Systems","Equipment Related","5.35","Medium","","","push button fixed and secured.","2021-01-01T23:59:35","","Completed","2020-12-30T23:59:35","No","No","No","Internal"]
[null,null,null,17448,null,"27_16/01/2021 8:57:50 PM","2020-12-18T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","rudder angle indicator error","Navigation - Others","Eng. / Strg. Comp.","Equipment Related","10.39","High","","","error adjusted ","2021-01-27T23:59:35","","Completed","2021-01-10T23:59:35","No","No","No","Internal"]
[null,null,null,17449,null,"27_16/01/2021 9:14:11 PM","2020-12-18T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","stern tube tank to mark normal LO level","Hull & Tanks","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Normal LO level marked on the tank.","2020-12-27T23:59:35","","Completed","2020-12-24T23:59:35","No","No","No","Internal"]
[null,null,null,17450,null,"27_16/01/2021 9:30:48 PM","2020-12-18T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ME RPLS SYSTEM SLIGHT OIL LEAKAGE","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.19","Very High","","","LEAK RECTIFIED.","2021-01-27T23:59:35","","Completed","2020-12-29T23:59:35","No","No","No","Internal"]
[null,null,null,17451,null,"27_16/01/2021 9:40:16 PM","2020-12-18T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ME FWD MANOMETER WATER NOT VISIBLE. NO KNOB FOUND","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.19","Very High","","","WATER FILLED UP . KNOB RENEWED","2021-01-01T23:59:35","","Completed","2020-12-28T23:59:35","No","No","No","Internal"]
[null,null,null,17452,null,"27_16/01/2021 9:43:48 PM","2020-12-18T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ME FWD SIDE MAN. PLATFORM OIL LEAK\t","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.19","Very High","","","OIL LEAK RECTIFIED. FLANGE GASKET RENEWED . NO LEAK","2021-01-13T23:59:35","","Completed","2020-12-23T23:59:35","No","No","No","Internal"]
[null,null,null,17453,null,"27_16/01/2021 9:46:43 PM","2020-12-18T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ME T/C NO.1 TACHOMETER ERROR","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","TACHOMETER ERROR ADJUSTED.","2020-12-31T23:59:35","","Completed","2021-12-24T23:59:35","No","No","No","Internal"]
[null,null,null,17454,null,"27_16/01/2021 9:49:38 PM","2020-12-18T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","220V AND 440 V LOW INSULATION IN EMERGENCY DG ROOM","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.38","Medium","","","LOW INSULATION RECTIFIED. NOW INFINITY","2020-12-27T23:59:35","","Completed","2020-12-20T23:59:35","No","No","No","Internal"]
[null,null,null,17455,null,"27_16/01/2021 9:52:39 PM","2020-12-18T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","PURIFIER ROOM SLUDGE TANK SOUNDING PIPE CAP MISSING","E/R - Purifier","Eng. / Strg. Comp.","Equipment Related","8.38","Medium","","","MISSING CAP RENEWED","2021-01-28T23:59:35","","Completed","2020-12-27T23:59:35","No","No","No","Internal"]
[null,null,null,17456,null,"27_16/01/2021 9:55:06 PM","2020-12-18T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","AE FO LINE VALVE HAND WHEEL MISSING","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","HANDWHEEL RENEWED WITH SPARE HANDWHEEL","2021-02-01T23:59:35","","Completed","2020-12-24T23:59:35","No","No","No","Internal"]
[null,null,null,17457,null,"27_16/01/2021 9:06:50 PM","2020-12-18T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","em generator FO tank save all tray has oil - to check source of leak.\t\t","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.35","Very High","","","leak rectified and area cleaned. No leak observed.","2021-01-27T23:59:35","","Completed","2020-12-29T23:59:35","No","No","No","Internal"]
[null,null,null,17458,null,"27_16/01/2021 10:02:28 PM","2020-12-18T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","FW HYDROPHORE LINE EGB WASHING TO BE CAPPED","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","8.38","Medium","","","LINE RENEWED WITH NEW CAP.","2021-01-27T23:59:35","","Completed","2020-12-28T23:59:35","No","No","No","Internal"]
[null,null,null,17459,null,"27_16/01/2021 10:07:24 PM","2020-12-18T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","FIRE ALARM MANUAL CALL POINT NEAR ENGINE ROOM ENTRANCE DOOR COVERED WITH PLASTIC","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","PLASTIC REMOVED AND ALL OTHER PANELS CHECKED.","2020-12-27T23:59:35","","Completed","2020-12-25T23:59:35","No","No","No","Internal"]
[null,null,null,17460,null,"27_16/01/2021 10:10:04 PM","2020-12-18T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","AE 3 CRANLKCASE VENT LINE FLANGE LEAKING","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.19","Very High","","","LEAK RECTIFIED. FLANGE BOLTS TIGHTENED AS THEY WERE LOOSE","2020-12-27T23:59:35","","Completed","2020-12-23T23:59:35","No","No","No","Internal"]
[null,null,null,17461,null,"27_16/01/2021 9:36:41 PM","2020-12-18T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Ship Staff Insp.","ME AIR COOLER FWD SLIGHT WATER LEAKAGE","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.19","Very High","","","LEAK RECTIFIED. GASKET RENEWED FOR THE FLANGE","2021-01-27T23:59:35","","Completed","2020-12-29T23:59:35","No","No","No","Internal"]
[null,null,null,17462,null,"27_16/01/2021 10:11:55 PM","2020-12-18T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ER FIRE HYDRANT AT EGB DECK CAP MISSING","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","8.38","Medium","","","CAP RENEWED WITH SPARE CAP","2021-01-27T23:59:35","","Completed","2020-12-23T23:59:35","No","No","No","Internal"]
[null,null,null,17463,null,"27_16/01/2021 9:59:01 PM","2020-12-18T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","INSULATION MAT TO RENEW FOR BWTS PANEL AND JCW HEATER PANEL","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.24","Low","","","MATS TO BE RENEWED WITH SPARE NEW MATS.","2021-01-28T23:59:35","","Completed","2020-12-28T23:59:35","No","No","No","Internal"]
[null,null,null,16654,null,"27_24/12/2020 10:36:21 AM","2020-12-19T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Aft hyd.system lube oil cooler sea water inlet pipe holed at 2 -places","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","PIPE RENEWED WITH SPARE NEW PIPE. SATISFACTORY..","2021-03-18T23:59:35","","Completed","2020-12-24T23:59:35","No","No","No","Internal"]
[null,null,null,17689,null,"27_02/02/2021 1:40:03 PM","2020-12-19T23:59:35","Observation","Ship Staff","Ship Staff Insp.","PORT/STBD ANCHOR LASHING WIRE FOUND DAMAGED WITH BROKEN STRANDS.","Deck - Pipe / Fittings","General Appearance","Behaviour Based,Equipment Related","9.2","Very High","","","NEW WIRES RECEIVED AT PORT SUEZ. SAME REPLACED AND SECURED.","2021-03-19T23:59:35","","Completed","2021-01-11T23:59:35","No","No","No","Internal"]
[null,null,null,17438,null,"27_15/01/2021 10:27:26 PM","2020-12-19T23:59:35","Defect,Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","MAIN DECK HOUSEKEEPING TO BE IMPROVED.","Miscellaneous","General Appearance","Behaviour Based,External Factors","11.3","Medium","","","MAIN DECK DERUSTING AND PAINITNG CARRIED OUT. STORES ARRANGED AND CLEANED.","2021-06-19T23:59:35","","Completed","2021-05-15T23:59:35","No","No","No","Internal"]
[null,null,null,17439,null,"27_15/01/2021 10:20:35 PM","2020-12-19T23:59:35","Defect,Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","SLOP (P) COT STEAM LINE AND HEATING COIL RUSTED.\t","Deck - Pipe / Fittings","General Appearance","Behaviour Based,External Factors","8.41","Medium","","","SLOP(P) HEATING COIL AND STEAM LINE DE-RUSTED & FULLY PAINTED.","2021-03-20T23:59:35","","Completed","2021-01-14T23:59:35","No","No","No","Internal"]
[null,null,null,17440,null,"27_15/01/2021 10:31:09 PM","2020-12-19T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","P/V BREAKER GAUGE GLASS  SPRING LOADED COCK FROZEN\t","Inert Gas","Cargo / Ballast Systems","Behaviour Based,Equipment Related","8.28","Medium","","","P/V BREAKER WATER/GLYCOL MIXTURE REPLENISHED. GAUGE GLASS COCK SPRING CLEANED, GREASED AND EXERCISED. NOW OPERATING SMOOTHLY.","2021-03-19T23:59:35","","Completed","2021-01-14T23:59:35","No","No","No","Internal"]
[null,null,null,17441,null,"27_15/01/2021 10:34:41 PM","2020-12-19T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","FEW MANIFOLD DRIP TRAY GRATINGS NOT SECURED.","Deck - Pipe / Fittings","General Appearance","Behaviour Based,Human Error","6.6","Medium","","","MANIFOLD DRIP TRAY GRATINGS CLAMPED AND SECURED.","2021-03-19T23:59:35","","Completed","2021-01-13T23:59:35","No","No","No","Internal"]
[null,null,null,17442,null,"27_15/01/2021 10:43:34 PM","2020-12-19T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","PORT & STBD ANCHOR CHAIN BITTER END HAMMERS NOT IN PLACE.","Deck - Pipe / Fittings","General Appearance","Behaviour Based,Human Error","9.22","Low","","","BITTER END HAMMERS PAINTED BRIGHT RED AND PLACED NEAR PORT/STBD CHAIN LOCKER.","2021-03-19T23:59:35","","Completed","2021-12-22T23:59:35","No","No","No","Internal"]
[null,null,null,17443,null,"27_15/01/2021 10:49:26 PM","2020-12-19T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","COW LINE UNDERSIDE AND SPACES I.W.O OF U-CLAMPS TO RUSTED.","Deck - Pipe / Fittings","General Appearance","Behaviour Based,Equipment Related","8.34","High","","","Completed","2021-10-19T23:59:35","","Completed","2021-09-01T23:59:35","No","No","No","Internal"]
[null,null,null,17444,null,"27_15/01/2021 10:55:23 PM","2020-12-19T23:59:35","Defect,Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","FORECASTLE DECK OLDMAN ROLLERS FROZEN.","Deck - Pipe / Fittings","General Appearance","Behaviour Based,External Factors","9.18","Low","","","FORECASTLE ROLLERS FULLY OPENED AND REMOVED. DE-RUSTING, PAINTING AND GREASING DONE. FOUND MOVING FREELY. ALL OLDMAN ROLLERS AND STAND ROLLERS GREASED. SATISFACTORY.","2021-03-19T23:59:35","","Completed","2021-02-22T23:59:35","No","No","No","Internal"]
[null,null,null,17445,null,"27_15/01/2021 10:58:29 PM","2020-12-19T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","MOORING WINCH NO.01 AND NO.05 SIGHT GLASS OPAQUE AND DIRTY.","Deck - Mooring Machinery","General Appearance","Equipment Related","9.14","Medium","","","SIGHT GLASS CHECKED AND CLEANED. ","2021-03-19T23:59:35","","Completed","2021-01-12T23:59:35","No","No","No","Internal"]
[null,null,null,17464,null,"27_15/01/2021 10:39:03 PM","2020-12-19T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","FORWARD WINDLASS HYDRAULIC PUMP NO.02 AMPERE METER NOT AT ZERO EVEN THOUGH THE PUMP IS STOPPED.","Deck - Mooring Machinery","Mooring","Equipment Related","9.14","Medium","","","AMPERE METER ADJUSTED AND SET TO ZERO.","2021-03-19T23:59:35","","Completed","2020-12-22T23:59:35","No","No","No","Internal"]
[null,null,null,16655,null,"27_04/01/2021 6:22:55 PM","2020-12-21T23:59:35","Defect","Ship Staff","Ship Staff Insp.","LEAK OBSERVED FROM THE CRANE HOISTING LEVER HOSE CONNECTIONS","Deck - Machinery","Emgcy. Systems","Equipment Related","8.5","Very High","","","DAMAGED ORINGS REPLACED AND LEAK RECTIFIED.","2021-01-10T23:59:35","","Completed","2020-12-28T23:59:35","No","No","No","Internal"]
[null,null,null,16656,null,"27_04/01/2021 6:19:22 PM","2020-12-25T23:59:35","Defect","Ship Staff","Ship Staff Insp.","1C COT IG INLET VALVE ACTUATOR DAMAGED DUE TO BROKEN STUDS","Inert Gas","Cargo / Ballast Systems","Behaviour Based,Equipment Related","8.1","Very High","","","ACTUATOR REPAIRED, OVERHAULED, NEW STUDS FIXED AND GREASED.","2021-01-10T23:59:35","","Completed","2020-12-27T23:59:35","No","No","No","Internal"]
[null,null,null,16649,null,"27_04/01/2021 6:27:03 PM","2020-12-27T23:59:35","Defect","Ship Staff","Ship Staff Insp.","MANIFOLD PRESSURE GAUGE BOX DAMAGED DUE TO WASTAGE.","Deck - Pipe / Fittings","General Appearance","Equipment Related,External Factors","8.21","High","","","NEW PRESSURE GAUGE BOX'S FABRICATED AND FIXED.","2021-03-27T23:59:35","","Completed","2021-01-27T23:59:35","No","No","No","Internal"]
[null,null,null,16657,null,"27_04/01/2021 4:14:49 PM","2020-12-27T23:59:35","Observation","Ship Staff","Ship Staff Insp.","DG NO.3 SUMP OIL TO RENEWE. DEFLECTION TO BE TAKEN AND TAPPET CLEARANCE TO BE ADJUSTED.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","SUMP OIL RENEWED WITH FRESH OIL. TAPPET CLEARANCE TAKEN AND ADJUSTED. DEFLECTION RECORDED. ALL FOUND SATISFACTORY.","2020-12-31T23:59:35","","Completed","2020-12-28T23:59:35","No","No","No","Internal"]
[null,null,null,17690,null,"27_02/02/2021 1:30:37 PM","2020-12-27T23:59:35","Defect,Observation","Ship Staff","Ship Staff Insp.","FORECASTLE STORE WEATHER TIGHT DOOR PACKING FOUND DAMAGED.","Deck - Pipe / Fittings","General Appearance","Behaviour Based,Equipment Related","11.6","Medium","","","DOOR PACKING METAL GROOVE CHIPPED/PAINTED AND NEW PACKING FITTED. VERIFIED PROPER SEALING. ","2021-03-27T23:59:35","","Completed","2021-01-07T23:59:35","No","No","No","Internal"]
[null,null,null,17691,null,"27_02/02/2021 1:52:36 PM","2020-12-27T23:59:35","Defect","Ship Staff","Ship Staff Insp.","SECURING SCBA BOTTLE HOLDER FOR ONE OF THE BA SET FOUND BROKEN.","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.43","High","","","NEW SECURING BOTTLE HOLDER FABRICATED AND FIXED FOR THE BA SET.","2021-03-27T23:59:35","","Completed","2020-12-28T23:59:35","No","No","No","Internal"]
[null,null,null,13434,null,"27_05/08/2020 4:52:55 AM","2020-12-27T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Drafts gauges reading were compared between actual draft and SAAB drafts and found large difference upto 60 cm at fwd / aft and mid drafts. ","Hull & Tanks,Miscellaneous","Cargo / Ballast Systems","Equipment Related","11.6","Medium","","","It is repeative defect,hence closing out.","2021-12-23T23:59:35","","Completed","2021-09-20T23:59:35","No","No","No","Internal"]
[null,null,null,16658,null,"27_04/01/2021 4:31:36 PM","2020-12-28T23:59:35","Observation","Ship Staff","Ship Staff Insp.","DG NO.1 CRANKCASE RELIEF DOORS FOUND TO BE LEAKING.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","CRANKCASE RELIEF DOORS O RINGS REPLACED . DG TRIED OUT . NO LEAKS OBSERVED. SATISFACTORY.","2020-12-30T23:59:35","","Completed","2020-12-30T23:59:35","No","No","No","Internal"]
[null,null,null,16652,null,"27_04/01/2021 4:28:24 PM","2020-12-29T23:59:35","Defect","Ship Staff","Ship Staff Insp.","IG FAN NO.2 DELIVERY VALVE SOLENOID ASSEMBLY FOUND TO BE LEAKING CASING SLUGISH OPERATION OF THE VALVE","Inert Gas","Eng. / Strg. Comp.","Equipment Related","8.22","Very High","","","valves ohauled ,tested satisfactory.","2021-03-28T23:59:35","","Completed","2021-03-18T23:59:35","No","No","No","Internal"]
[null,null,null,17684,null,"27_31/01/2021 12:14:25 AM","2020-12-29T23:59:35","Observation","Ship Staff","Ship Staff Insp.","STERILIZER UV LAMP QUARTZ TUBE BROKEN. NEED TO REPLACE IT","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","12.8","High","","","QUARTZ TUBE  REPLACED WITH NEW RCVD.","2021-03-27T23:59:35","DLOT210020","Completed","2021-03-16T23:59:35","No","No","No","Internal"]
[null,null,null,17692,null,"27_27/01/2021 11:17:21 PM","2020-12-29T23:59:35","Observation","Ship Staff","Ship Staff Insp.","PURIFIER ROOM EXHAUST FAN DAMPER ASSEMBLY AIR UNIT FOUND TO BE LEAKING. NEED TO BE OVERHAULED AND O RING TO RENEW","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","DAMPER ASSEMBLY OVERHAULED WITH NEW O RINGS. NO MORE LEAK FOUND","2021-01-27T23:59:35","","Completed","2021-01-15T23:59:35","No","No","No","Internal"]
[null,null,null,17465,null,"27_16/01/2021 10:14:43 PM","2020-12-29T23:59:35","Observation","Ship Staff","Ship Staff Insp.","EMERGECNY FIRE PUMP MOTOR AND PUMP OVERHAUL","Critical Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","MOTOR AND PUMP OVERHAULED. FOUND TO BE SATISFACTORY.","2021-01-07T23:59:35","","Completed","2021-01-07T23:59:35","No","No","No","Internal"]
[null,null,null,17765,null,"27_12/02/2021 11:24:19","2020-12-29T23:59:35","Critical Equipment,Defect","Ship Staff","Ship Staff Insp.","PM TEST OF  S-BAND RADAR; THE READINGS SHOWN BY THE PM TEST INDICATES DEGRADATION OF RADAR’S PERFORMANCE TX System\n\nBar display: 2.9\n\nAtt Value: (-) 15.0 Db\n\n","Navigation - RADAR","Navigation","Equipment Related","4.2","Medium","","","NEW RADAR INSTALLED","2021-05-25T23:59:35","","Completed","2021-04-25T23:59:35","No","No","No","Internal"]
[null,null,null,17693,null,"27_02/02/2021 2:22:18 PM","2020-12-30T23:59:35","Observation","Ship Staff","Ship Staff Insp.","SECURING ARRANGEMENT FOR FEW HYDRANT CAPS ON DECK & E/ROOM WERE MISSING.","LSA / FFA","Safety / LSA / FFA","Behaviour Based","5.38","High","","","ALL HYDRANTS WERE CHECKED AND CAPS FIXED WITH SECURING ARRANGEMENTS.","2021-03-30T23:59:35","","Completed","2021-01-10T23:59:35","No","No","No","Internal"]
[null,null,null,17694,null,"27_02/02/2021 1:45:00 PM","2020-12-31T23:59:35","Defect","Ship Staff","Ship Staff Insp.","VECS PRESSURE SENSOR GIVING ERRATIC READINGS.","Inert Gas","Cargo / Ballast Systems","Equipment Related","9.19","Low","","","PRESSURE SENSOR CABINET WAS OPENED, CLEANED DRY FOR MOISTURE AND SEALENT APPLIED TO AVOID WATER INGRESS. PRESSURE VERIFIED AND MATCHING WITH MAIN LINE PRESSURE.","2021-03-31T23:59:35","","Completed","2021-01-06T23:59:35","No","No","No","Internal"]
[null,null,null,17695,null,"27_27/01/2021 11:18:43 PM","2021-01-02T23:59:35","Observation","Ship Staff","Ship Staff Insp.","BOTH BOILER GAUGE GLASS TO OVERHAUL","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","GAUGE GLASS OVERHAULED AND DRAIN LINES CLEARED.","2021-01-27T23:59:35","","Completed","2021-01-18T23:59:35","No","No","No","Internal"]
[null,null,null,17696,null,"27_02/02/2021 1:36:37 PM","2021-01-02T23:59:35","Defect","Ship Staff","Ship Staff Insp.","GAS DETECTION AUDIBLE ALARM IN PUMPROOM FOUND IN-OPERATIONAL.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","5.22","High","","","ALARM RECTIFIED AND TRIED OUT. FOUND OPERATIONAL.","2021-04-02T23:59:35","","Completed","2021-01-23T23:59:35","No","No","No","Internal"]
[null,null,null,17697,null,"27_27/01/2021 11:11:56 PM","2021-01-08T23:59:35","Defect,Observation","Ship Staff","Ship Staff Insp.","ME LO PURIFIER 4000HRS BOWL CLEANING ROUTINE.","E/R - Purifier","Eng. / Strg. Comp.","Equipment Related","","","","","4000HRS ROUTINE CARRIED OUT. PURIFIER RUNNING SATISFACOTRY.","2021-01-28T23:59:35","","Completed","2021-01-09T23:59:35","No","No","No","Internal"]
[null,null,null,17685,null,"27_27/01/2021 11:20:42 PM","2021-01-10T23:59:35","Defect,Observation","Ship Staff","Ship Staff Insp.","VERY SLIGHT LEAK IN STERN TUBE FWD SEAL.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.19","Very High","","","VERY MINOR LEAKAGE OBSERVED FOUND WITHIN MAKERS ALLOABLE LIMIT SAME WILL B ETRANSFERRED TO REFMAN FO RNEXT DD","2021-04-09T23:59:35","","Completed","2021-04-10T23:59:35","No","No","No","Internal"]
[null,null,null,17698,null,"27_02/02/2021 1:20:47 PM","2021-01-10T23:59:35","Defect","Ship Staff","Ship Staff Insp.","LEAK OBSERVED FROM HOISTING RUBBER HOSE CONNECTOR. ","Deck - Machinery","General Appearance","Equipment Related","8.5","Very High","","","LEAK WAS REPAIRED BY REPLACING THE DAWTY SEAL ON THE HOSE CONNECTOR.","2021-04-10T23:59:35","","Completed","2021-01-11T23:59:35","No","No","No","Internal"]
[null,null,null,17686,null,"27_27/01/2021 11:14:46 PM","2021-01-12T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","FIRE AND GS PPUMP MOTOR BURNT DURING NORMAL RUNNING.","LSA / FFA","Eng. / Strg. Comp.","Equipment Related","10.24","Low","","","MOTOR TO BE REPLACED ONCE SPARE MOTOR RECEIVED. PUMP ALSO OVERHAULED","2021-02-15T23:59:35","DLOT210023","Completed","2021-02-09T23:59:35","No","No","No","Internal"]
[null,null,null,17699,null,"27_02/02/2021 1:47:50 PM","2021-01-12T23:59:35","Defect,Observation","Ship Staff","Ship Staff Insp.","STBD SIDE AFT BUNKER MANIFOLD PRESSURE GAUGE FOUND BROKEN.","Deck - Pipe / Fittings","General Appearance","Equipment Related","8.41","Medium","","","NEW PRESSURE GAUGE FIXED.","2021-04-12T23:59:35","","Completed","2021-01-21T23:59:35","No","No","No","Internal"]
[null,null,null,17700,null,"27_02/02/2021 2:26:08 PM","2021-01-14T23:59:35","Defect","Ship Staff","Ship Staff Insp.","LOW EXPANSION FOAM DRAIN LINE VALVE SPINDLE FOUND BROKEN.","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.38","High","","","NEW FOAM LINE DRAIN VALVE FIXED.","2021-04-14T23:59:35","","Completed","2021-01-18T23:59:35","No","No","No","Internal"]
[null,null,null,17701,null,"27_25/01/2021 12:17:22 PM","2021-01-15T23:59:35","Observation","Ship Staff","Ship Staff Insp.","MOORING WINCH M6 OPERATING LEVER FOUND LEAKING","Deck - Mooring Machinery","Mooring","Equipment Related","9.14","Medium","","","OPERATING LEVER BLOCK WAS REMOVED AND O-RING WAS REPLACED. WINCH TRIED OUT AND NO LEAKS OBSERVED.","2021-04-15T23:59:35","","Completed","2021-01-18T23:59:35","No","No","No","Internal"]
[null,null,null,17702,null,"27_02/02/2021 1:16:29 PM","2021-01-15T23:59:35","Defect","Ship Staff","Ship Staff Insp.","HYDRAULIC BRAKE CYLINDER FOR M3(A) MOORING WINCH FOUND LEAKING.","Deck - Mooring Machinery","General Appearance","Equipment Related","9.14","Medium","","","NEW HYDRAULIC CYLINDER FIXED FOR M3(A) WINCH, BRC TEST DONE AT 69T AND TRIED OUT SATISFACTORILY.","2021-04-15T23:59:35","","Completed","2021-01-20T23:59:35","No","No","No","Internal"]
[null,null,null,17687,null,"27_27/01/2021 11:23:08 PM","2021-01-17T23:59:35","Observation","Ship Staff","Ship Staff Insp.","TDC SENSOR FOR DOCTOR FOUND TO BE DEFECTIVE. SAME TO BE RENEWED ONCE MAIN ENGINE STOPS.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","TDC SENSOR RENEWED WITH SPARE SENSOR.","2021-02-07T23:59:35","","Completed","2021-02-02T23:59:35","No","No","No","Internal"]
[null,null,null,17703,null,"27_03/02/2021 12:22:45 AM","2021-01-17T23:59:35","Observation","Ship Staff","Ship Staff Insp.","DO TRANSFER PUMP MOTOR OVERHAULING TO BE CARREID OUT.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","MOTOR OVERHAULED AND FOUND TO BE WORKING SATISFACOTRY.","2021-01-27T23:59:35","","Completed","2021-01-20T23:59:35","No","No","No","Internal"]
[null,null,null,17704,null,"27_02/02/2021 1:55:56 PM","2021-01-18T23:59:35","Observation","Ship Staff","Ship Staff Insp.","CRADLES FOR STOWING LIFERAFTS FOUND DETERIORATED DUE TO RUST AND WASTAGE.","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.28","Very High","","","DE-RUSTING DONE ON THE CRADLES, PAINTED AND RELEASE PINS GREASED.","2021-04-18T23:59:35","","Completed","2021-01-23T23:59:35","No","No","No","Internal"]
[null,null,null,17705,null,"27_02/02/2021 1:13:02 PM","2021-01-19T23:59:35","Defect","Ship Staff","Ship Staff Insp.","OPERATING LEVER OF M5 MOORING WINCH NOT MOVING SMOOTHLY DUE TO ALIGNMENT ISSUE.","Deck - Mooring Machinery","General Appearance","Equipment Related","9.14","Medium","","","OPERATING LEVER BLOCK WAS REMOVED, O-RINGS REPLACED AND ALIGNED. OPERATING LEVER AND MOVEMENT OF WINCH TRIED OUT SATISFACTORILY","2021-04-19T23:59:35","","Completed","2021-01-21T23:59:35","No","No","No","Internal"]
[null,null,null,17706,null,"27_03/02/2021 12:18:55 AM","2021-01-20T23:59:35","Observation","Ship Staff","Ship Staff Insp.","FW HYDROPHORE MOTOR NO.1 OVERHAULING","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","MOTOR OVERHAULED. BEARINGS RENEWED. RUNNING SATISFACOTRY.","2021-01-28T23:59:35","","Completed","2021-01-22T23:59:35","No","No","No","Internal"]
[null,null,null,17688,null,"27_03/02/2021 12:15:57 AM","2021-01-24T23:59:35","Defect","Ship Staff","Ship Staff Insp.","WMES 002 SAMPLING PUMP MOTOR INSULATION FOUND TO BE VERY LOW. 220V MOTOR TO BE RENEWED.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.24","Low","","","Spare pp  rcvd and replaced.","2021-04-23T23:59:35","DLOT210032","Completed","2021-03-26T23:59:35","No","No","No","Internal"]
[null,null,null,17774,null,"27_14/02/2021 12:51:54 PM","2021-01-27T23:59:35","Defect,Observation","Ship Staff","Ship Staff Insp.","AFT ROPE HATCH OPENING COVER DAMAGED DUE TO WASTAGE.","Deck - Pipe / Fittings","General Appearance","Behaviour Based","11.6","Medium","","","AFT ROPE HATCH COVER REPAIRED, HIGES FABRICATED, DE-RUSTED AND FIXED.","2021-04-26T23:59:35","","Completed","2021-02-06T23:59:35","No","No","No","Internal"]
[null,null,null,17775,null,"27_14/02/2021 12:55:01 PM","2021-01-27T23:59:35","Defect","Ship Staff","Ship Staff Insp.","GALLEY OVEN DOOR HINGES BROKEN.\t","Accommodation","General Appearance","Behaviour Based","11.13","Low","","","OVEN DOOR HINGES FABRICATED AND FIXED.","2021-04-26T23:59:35","","Completed","2021-02-07T23:59:35","No","No","No","Internal"]
[null,null,null,17777,null,"27_14/02/2021 6:58:29 PM","2021-01-29T23:59:35","Observation","Ship Staff","Ship Staff Insp.","ALL ENGINE ROOM BILGES FOUND TO BE DIRTY.\t","Hull & Tanks","Eng. / Strg. Comp.","Equipment Related","8.44","High","","","ALL BILGE WELLS EMPTIED OUT , CLEANED AND COATED WITH PAINT","2021-02-24T23:59:35","","Completed","2021-02-07T23:59:35","No","No","No","Internal"]
[null,null,null,17766,null,"27_14/02/2021 1:35:28 PM","2021-02-05T23:59:35","Defect","Ship Staff","Ship Staff Insp.","METAL COVER EDGES FOR COVERING THE TUBE FOR FIXED GAS DETECTION PIPING DAMAGED DUE TO WASTAGE ON FWD MAIN DECK.","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.4","Very High","","","METAL COVERS TO CROPPED, FABRICATED & PAINTED.","2021-05-05T23:59:35","","Completed","2021-03-10T23:59:35","No","No","No","Internal"]
[null,null,null,17767,null,"27_14/02/2021 1:42:54 PM","2021-02-05T23:59:35","Observation","Ship Staff","Ship Staff Insp.","EXCESS RUST ON MOORING WINCHES AFT ESPECIALLY ON THE FOUNDATION AND SUPPORTS.","Deck - Mooring Machinery","General Appearance","Equipment Related","9.14","Medium","","","HYDROBLASTING, BUFFING, PAINTING OF THE MOORING WINCHES AFT & POOP DECK COMPLETED. STENCILS & MARKINGS DONE.","2021-05-05T23:59:35","","Completed","2021-03-18T23:59:35","No","No","No","Internal"]
[null,null,null,17768,null,"27_15/02/2021 4:57:26 AM","2021-02-05T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Purifier room sludge tank vent pipe partially clogged ","E/R - Pipes/ valves & fittings,E/R - Purifier,Hull & Tanks","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","One pipe section removed  and found clean condition.","2021-05-04T23:59:35","","Completed","2021-03-11T23:59:35","No","No","No","Internal"]
[null,null,null,17769,null,"27_14/02/2021 1:15:25 PM","2021-02-07T23:59:35","Critical Equipment,Defect,Non Conformity","Ship Staff","Ship Staff Insp.","FIXED CO2 RELEASE CABINET FOR ECR IN FIRE CONTROL STATION FOUND BROKEN FROM BASE AND FALLEN DOWN. CAUSE APPEARS TO BE THE DETERIORATION IN THE QUALITY OF PLASTIC CABINET OVER A PERIOD OF TIME.","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.4","High","","","NEW CABINET FABRICATED FOR THE PILOT BOTTLES, PAINTED SIGNAL RED AND FIXED IN THE FIRE CONTROL STATION","2021-05-07T23:59:35","","Completed","2021-02-08T23:59:35","No","No","No","Internal"]
[null,null,null,17776,null,"27_14/02/2021 7:07:05 PM","2021-02-07T23:59:35","Breakdown,Defect","Ship Staff","Ship Staff Insp.","CO2 PILOT CYLINDER CABINET FOR ECR IN FIRE STATION FOUND TO HAVE BROKEN DOWN. NEED TO FABRICATE NEW.","Critical Equip.","Emgcy. Systems","Equipment Related","5.35","Medium","","","NEW BOX FABRICATED AND INSTALLED. SATISFACOTRY.","2021-02-11T23:59:35","","Completed","2021-02-09T23:59:35","No","No","No","Internal"]
[null,null,null,17770,null,"27_14/02/2021 2:56:04 PM","2021-02-08T23:59:35","Defect","Ship Staff","Ship Staff Insp.","MANUAL HYDRAULIC SUCTION VALVE FOR FPK VOID TANK UNABLE TO OPEN, SUSPECT STUCK IN CLOSED POSITION.","Deck - Pipe / Fittings","General Appearance","Equipment Related","8.61","Medium","","","VALVE OVERHAULED, SEALS RENEWED. TRIED OUT SATISFACTORILY.","2021-05-08T23:59:35","","Completed","2021-02-13T23:59:35","No","No","No","Internal"]
[null,null,null,17771,null,"27_14/02/2021 3:02:40 PM","2021-02-08T23:59:35","Defect","Ship Staff","Ship Staff Insp.","FPK VOID TANK SPACE EDUCTOR LIQUID DRIVING MANUAL GATE VALVE (BGV04) FOUND NOT HOLDING. ","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.61","Medium","","","VALVE RENEWED AND TRIED OUT. NO LEAKS OBSERVED. SATISFACTORY.","2021-05-08T23:59:35","","Completed","2021-02-13T23:59:35","No","No","No","Internal"]
[null,null,null,17772,null,"27_14/02/2021 7:18:41 PM","2021-02-08T23:59:35","Observation","Ship Staff","Ship Staff Insp.","LINER WALL TEMP VALVE /ACTUATOR FOUND TO BE IN STUCK IN OPEN  COOLING WATER SIDE POSITION. NO RESPONSE BY THE ACTUATOR DURING CHANGE OF LOAD ON MAIN ENGINE.","E/R - Main Engine,E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.19","Very High","","","3WAY VALVE FOR LINER TEMP CONTROLLER EASED UP AND MOVEMENT CHECKED ALL SATISFACTORY.","2021-05-07T23:59:35","","Completed","2021-04-05T23:59:35","No","No","No","Internal"]
[null,null,null,18068,null,"27_22/02/2021 7:41:05 PM","2021-02-08T23:59:35","Observation","Ship Staff","Ship Staff Insp.","BILGE HOLDING TANK FOUND TO BE DIRTY. REQUIRES CLEANING","Hull & Tanks","Eng. / Strg. Comp.","Equipment Related","8.44","High","","","BILGE HOLDING TANK TO BE CLEANED.","2021-02-24T23:59:35","","Completed","2021-02-13T23:59:35","No","No","No","Internal"]
[null,null,null,17773,null,"27_14/02/2021 7:10:51 PM","2021-02-09T23:59:35","Observation","Ship Staff","Ship Staff Insp.","STEAM HEATING VALVE FOR DECK FOUND TO BE LEAKING .(NOT HOLDING)","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","8.35","Medium","","","VALVE OPENED AND SHUT WITH \"F\" KEY. FOUND TO BE HOLDING.","2021-03-27T23:59:35","","Completed","2021-02-11T23:59:35","No","No","No","Internal"]
[null,null,null,18069,null,"27_22/02/2021 7:43:56 PM","2021-02-12T23:59:35","Observation","Ship Staff","Ship Staff Insp.","CLEAN DRAIN TANK FOUND TO BE DIRTY. SAME NEED TO BE CLEANED.","Hull & Tanks","Eng. / Strg. Comp.","Equipment Related","8.44","High","","","CLEAN DRAIN TANK CLEANED","2021-02-24T23:59:35","","Completed","2021-02-18T23:59:35","No","No","No","Internal"]
[null,null,null,18070,null,"27_25/02/2021 12:24:08 PM","2021-02-15T23:59:35","Defect","Ship Staff","Ship Staff Insp.","LEAK FROM PORT SIDE MIDSHIP CRANE SLEWING BLOCK AND HOISTING BLOCK CONNECTOR NOTICED.","Deck - Machinery","General Appearance","Equipment Related","8.5","Very High","","","LEAK RECTIFIED BY RENEWAL OF DAWTY SEAL ON THE SLEWING BLOCK CONNECTOR AND RENEWAL OF O-RING ON THE HOISTING BLOCK CONNECTORS. TRIED OUT, NO LEAKS OBSERVED. ","2021-05-15T23:59:35","","Completed","2021-02-19T23:59:35","No","No","No","Internal"]
[null,null,null,18071,null,"27_25/02/2021 12:18:23 PM","2021-02-16T23:59:35","Defect","Ship Staff","Ship Staff Insp.","PUMPROOM BILGE SUCTION MAIN VALVE (207), WHICH IS A MANUALLY OPERATED HYDRAULIC VALVE WAS NOT OPENING FULLY WHEN TRIED OUT","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.47","Very High","","","SAME HAS BEEN OVERHAULED, OIL REFILLED AND TRIED OUT SATISFACTORILY.","2021-05-16T23:59:35","","Completed","2021-02-19T23:59:35","No","No","No","Internal"]
[null,null,null,12906,null,"27_29/06/2020 10:26:56 PM","2021-02-23T23:59:35","Defect","Ship Staff","Ship Staff Insp.","FWG Heat exchanger bottom cover thinned/holed","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","8.35","Medium","","","bottom cover renewed.","2021-04-22T23:59:35","spares rcvd on board on 20th March 21","Completed","2021-04-04T23:59:35","No","No","No","Internal"]
[null,null,null,18065,null,"27_28/02/2021 3:49:21 AM","2021-02-23T23:59:35","Observation","Ship Staff","Ship Staff Insp.","While taking Inventory found main engine piston ring top =1pc and 2nd,3rd&4th rings ROB nil","E/R - Main Engine","Eng. / Strg. Comp.","Human Error","10.32","Very High","","","Spare rcvd on board on 20th March 21","2021-04-26T23:59:35","Spare rcvd","Completed","2021-03-15T23:59:35","No","No","No","Internal"]
[null,null,null,18066,null,"27_28/02/2021 3:52:41 AM","2021-02-23T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Main Engine  shaft earthing device meter reading ZERO always","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Spare slip ring rcvd and renewed.","2021-04-26T23:59:35","spares rcvd","Completed","2021-03-26T23:59:35","No","No","No","Internal"]
[null,null,null,18067,null,"27_01/03/2021 2:29:55 AM","2021-02-23T23:59:35","Defect","Ship Staff","Ship Staff Insp.","DG 1&2 OIL Max not operational as flexible hoses leaking.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Spares rcvd and renewed.","2021-05-27T23:59:35","DLOT210022 ","Completed","2021-03-15T23:59:35","No","No","No","Internal"]
[null,null,null,18324,null,"27_16/03/2021 7:29:17 PM","2021-02-28T23:59:35","Defect","Ship Staff","Ship Staff Insp.","SLP(P) STEAM INLET LINE AND BYPASS TRAP GASKET FOUND DAMAGED.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.15","High","","","GASKET RENEWED FOR STEAM INLET LINE & BYPASS TRAP.","2021-05-31T23:59:35","","Completed","2021-03-07T23:59:35","No","No","No","Internal"]
[null,null,null,23214,null,"27_30/12/2021 12:03:14 AM","2021-03-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Gyro panel , LCD screen flickering at all times and some times its not readable","Navigation - Others","Navigation","Equipment Related","","","","","HDM/OCM display panel renewed by service engineer","2022-03-01T23:59:35","DLOT220095","Completed","2022-02-16T23:59:35","No","No","No","Internal"]
[null,null,null,18322,null,"27_17/03/2021 10:34:09 AM","2021-03-05T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Jacket water leaking from unused lubricating quills flange of ME unit no. 2&5.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","O-ring and Packings renewed.","2021-06-25T23:59:35","DLOT210036","Completed","2021-03-27T23:59:35","No","No","No","Internal"]
[null,null,null,18679,null,"27_31/03/2021 4:46:45 PM","2021-03-05T23:59:35","Defect,Observation","Ship Staff","Ship Staff Insp.","LIFERAFT RAILINGS AND SECURING PINS FOUND STUCK DUE TO CORROSION","LSA / FFA","Safety / LSA / FFA","Behaviour Based,Equipment Related","","","","","THE RAILING ARRANGEMENT FOR LIFERAFT AND THE SECURING PIN WAS COMPLETELY DE-RUSTED AND GREASED. ALL LIFERAFT SECURING PINS GREASED AND THE RAILING ARRANGEMENTS CHECKED & FOUND SATISFACTORY.","2021-06-05T23:59:35","","Completed","2021-03-10T23:59:35","No","No","No","Internal"]
[null,null,null,18684,null,"27_31/03/2021 4:57:35 PM","2021-03-05T23:59:35","Defect,Observation","Ship Staff","Ship Staff Insp.","FORWARD LIFERAFT EMBARKATION GATE RAILINGS FOUND STUCK","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","THE GATE RAILINGS WERE COMPLETELY DE-RUSTED, PAINTED, GREASED & TRIED OUT FOR FREE MOVEMENT FROM THE HINGES. ","2021-06-05T23:59:35","","Completed","2021-03-07T23:59:35","No","No","No","Internal"]
[null,null,null,18323,null,"27_17/03/2021 10:38:49 AM","2021-03-06T23:59:35","Defect","Ship Staff","Ship Staff Insp.","FWD ICCP giving abnormal alarm, Ref Cell no.2 voltage showing 0mV.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.37","Medium","","","Vessel arrived at QINGDAO anchorage after checking wiring for loose connection fault reset its own exact reason not known","2021-04-10T23:59:35","","Completed","2021-03-26T23:59:35","No","No","No","Internal"]
[null,null,null,18680,null,"27_31/03/2021 5:01:08 PM","2021-03-15T23:59:35","Defect,Observation","Ship Staff","Ship Staff Insp.","BROKEN STRANDS OF MANILA ROPE ON LIFEBOAT PAINTERS & PUMPROOM RESCUE ARRANGEMENT","LSA / FFA","Safety / LSA / FFA","Behaviour Based,Equipment Related","5.28","Very High","","","THE MANILA ROPES FOR BOTH LIFEBOAT PAINTERS AND THE PUMPROOM RESCUE ARRANGEMENTS WERE REPLACED WITH A NEW MANILA ROPE.","2021-06-15T23:59:35","","Completed","2021-03-20T23:59:35","No","No","No","Internal"]
[null,null,null,18681,null,"27_31/03/2021 4:42:30 PM","2021-03-17T23:59:35","Non Conformity,Observation","Ship Staff","Ship Staff Insp.","STBD SIDE PUMPROOM FLOODING DAMPER FOUND NOT CLOSING SLIGHTLY WHEN OPERATED DUE TO PAINT ACCUMULATION ON THE FLAPS.","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.19","Medium","","","THE MESH WAS REMOVED, EXCESS PAINT WAS REMOVED, FLAPS GREASED, CHECKED FOR FREE MOVEMENT AND TRIED OUT.","2021-06-17T23:59:35","","Completed","2021-03-19T23:59:35","No","No","No","Internal"]
[null,null,null,18682,null,"27_31/03/2021 7:17:26 PM","2021-03-17T23:59:35","Observation","Ship Staff","Ship Staff Insp.","NO.04 FOAM MONITOR VALVE FOUND SLIGHTLY LEAKING","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","FOAM MONITOR VALVE REMOVED AND OVERHAULED. TRIED OUT AND NO LEAKS FOUND.","2021-06-17T23:59:35","","Completed","2021-03-20T23:59:35","No","No","No","Internal"]
[null,null,null,18672,null,"27_24/03/2021 8:19:49 AM","2021-03-19T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Onborad in accomodation and engine room tube lights total 275 nos were converted to LED but existing circuit did not modified starter and choke still in use.","Accommodation,Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related,Human Error","10.32","Very High","","","completed","2021-12-19T23:59:35","","Completed","2021-11-10T23:59:35","No","No","No","Internal"]
[null,null,null,18673,null,"27_31/03/2021 4:11:40 PM","2021-03-26T23:59:35","Defect","Ship Staff","Ship Staff Insp.","DG 3 Sump low level flaot in operational ,however high level working and it is combo flaot level switch","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.11","Medium","","","Level switch renewed ","2021-12-25T23:59:35","DLOT210075 iTEM NO 24","Completed","2021-12-07T23:59:35","No","No","No","Internal","Spares supplied earlier, when installed found not of correct type, hence awaiting correct spare which has a lead time of 90 days."]
[null,null,null,18674,null,"27_31/03/2021 4:15:27 PM","2021-03-26T23:59:35","Observation","Ship Staff","Ship Staff Insp.","DG 3 save all tray drains connected to clean bilge tank when ever leakage oil is going the tank ,as previously Turbogenerator was fitted same removed and diesel engine installed ,but drains were not re routed to waste oil or fuel oil drain tank","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Drains routed to waste oil tank.","2021-06-25T23:59:35","DLOT210092","Completed","2021-05-28T23:59:35","No","No","No","Internal"]
[null,null,null,18683,null,"27_06/04/2021 3:26:09 PM","2021-04-01T23:59:35","Observation","Ship Staff","Ship Staff Insp.","THE FLAPS FOR AIR INTAKE FOR MAIN ENGINE TURBOCHARGER ARE STUCK DUE TO RUST ON THE HINGES.\t","Miscellaneous","General Appearance","Equipment Related","11.6","Medium","","","ALL HINGES DERUSTED AND EASED UP AND LUBRICATED TO MADE FREE MOVEMENT","2021-07-01T23:59:35","","Completed","2021-04-08T23:59:35","No","No","No","Internal"]
[null,null,null,18675,null,"27_17/04/2021 4:12:31 PM","2021-04-07T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Fore mast anchor light failure alarm not operational.","Navigation - Others","Navigation","Equipment Related","4.8","Medium","","","Fore mast anchor light failure alarm not operational ,same truobleshoot in progress ,as observed modification has been done in past and wiring diagram not available onboard.","2021-07-06T23:59:35","","Completed","2021-06-23T23:59:35","No","No","No","Internal"]
[null,null,null,18063,null,"27_28/02/2021 3:41:21 AM","2021-04-10T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Main engine VIT actuator rod seal leaking.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Leaky seal renewed with spare rcvd,","2021-12-09T23:59:35","DLOT210099","Completed","2022-02-13T23:59:35","No","No","No","Internal","spares are ready and will be connected to vsl at next port."]
[null,null,null,24681,null,"27_04/03/2022 4:03:41 PM","2021-04-12T23:59:35","Observation","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","PAL PMS Individual Job Description not Recorded after Completion of Emergency Gen Load Test,ie Test Parameters.","Elect. Mach. & Equip.","ISM Related","Human Error","10.12","Very High","","","PAL PMS Job Description Updated after Completion of Emergency Gen Load Test,ie Test Parameters.","2021-04-25T23:59:35","NA","Completed","2021-04-13T23:59:35","No","No","No","External"]
[null,null,null,18676,null,"27_17/04/2021 2:56:25 PM","2021-04-12T23:59:35","Defect","Ship Staff","Ship Staff Insp.","BALLAST PP NO 1 lOWER BEARING TEMP SENSOR DAMAGED","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.19","High","","","Sensor renewed and now shows proper temp.","2021-10-11T23:59:35","DLOT210107","Completed","2021-09-30T23:59:35","No","No","No","Internal"]
[null,null,null,18677,null,"27_17/04/2021 3:16:37 PM","2021-04-12T23:59:35","Critical Equipment","Ship Staff","Ship Staff Insp.","Incinerator settling tank quick closing valve waste oil transfer pump missing","LSA / FFA","Safety / LSA / FFA","Equipment Related","10.17","Very High","","","Spare valve received and fitted in place.","2021-07-11T23:59:35","DLOT210106 ITEM NO 2","Completed","2021-06-08T23:59:35","No","No","No","Internal"]
[null,null,null,18671,null,"27_23/03/2021 8:44:52 PM","2021-04-18T23:59:35","Defect","Ship Staff","Ship Staff Insp.","AE3 fuel oil booster pump standby pressure switch is defective as its diaphragm is found to be damaged. Due to this a leak was observed by Duty Engineer while taking rounds in Engine room.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Pressure switch to be renewed once spare is received onboard","2021-10-15T23:59:35","RO no  DLOT210029  Item no 7","Completed","2021-09-30T23:59:35","No","No","No","Internal"]
[null,null,null,18940,null,"27_29/04/2021 5:20:50 PM","2021-04-18T23:59:35","Defect,Observation","Ship Staff","Ship Staff Insp.","STBD SIDE PROVISION CRANE HOOK SWIVEL FOUND STUCK. ","Deck - Machinery","General Appearance","Equipment Related","8.5","Very High","","","HOOK SWIVEL FOR BOTH CRANES GREASED, EXERCISED & CHECKED FOR FREE MOVEMENT.","2021-07-18T23:59:35","","Completed","2021-04-20T23:59:35","No","No","No","Internal"]
[null,null,null,18941,null,"27_29/04/2021 5:17:35 PM","2021-04-20T23:59:35","Defect","Ship Staff","Ship Staff Insp.","TWO LIGHT FITTINGS ON ENGINE CASING BLOCK UPP DECK FOUND TO BE BROKEN.","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.1","High","","","BROKEN FITTINGS WERE REPLACED WITH NEW FITTINGS.","2021-07-20T23:59:35","","Completed","2021-04-22T23:59:35","No","No","No","Internal"]
[null,null,null,18934,null,"27_29/04/2021 5:08:28 PM","2021-04-22T23:59:35","Defect","Ship Staff","Ship Staff Insp.","PUMPROOM EXHAUST FAN FLAP LEVER FOUND BROKEN DUE TO WASTAGE.","Deck - Pipe / Fittings","General Appearance","Equipment Related","5.18","High","","","LEVERS REPAIRED/FABRICATED FOR BOTH FLAPS AND FIXED BACK.","2021-07-22T23:59:35","","Completed","2021-05-01T23:59:35","No","No","No","Internal"]
[null,null,null,18935,null,"27_29/04/2021 5:54:39 PM","2021-04-22T23:59:35","Defect","Ship Staff","Ship Staff Insp.","FWD ICCP fault as “ Cell #2 under protection status   limit 10-450      0mV”","Hull & Tanks","Structural Condn. / WT integrity ","Equipment Related","10.11","Medium","","","Fwd ICCP is now functioning properly","2021-07-21T23:59:35","","Completed","2021-07-01T23:59:35","No","No","No","Internal"]
[null,null,null,18060,null,"27_28/02/2021 3:28:42 AM","2021-04-23T23:59:35","Observation","Ship Staff","Ship Staff Insp.","AE1  fuel valves are due for nozzle replacement","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","AE1  fuel valves nozzles  replaced  with spares ones.","2021-07-22T23:59:35","RO no DLOT210025 item no 10","Completed","2021-06-12T23:59:35","No","No","No","Internal"]
[null,null,null,18061,null,"27_28/02/2021 3:35:20 AM","2021-04-23T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Emergency generator hydraulic pump pressure drops after kept in STBY however no issue after raising pressure and starting the generator","Elect. Mach. & Equip.","Emgcy. Systems","Equipment Related","10.32","Very High","","","Spare Hyd.pump received ,fitted in place and found to be working satisfactory.","2021-07-22T23:59:35","DLOT210083","Completed","2021-06-09T23:59:35","No","No","No","Internal"]
[null,null,null,18064,null,"27_28/02/2021 3:44:28 AM","2021-04-23T23:59:35","Defect,Observation","Ship Staff","Ship Staff Insp.","Emergency fire pp room drain pipe clogged which is passing through the After peak tank","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","5.41","Very High","","","Drain pipe cleared.","2021-07-22T23:59:35","","Completed","2021-05-05T23:59:35","No","No","No","Internal"]
[null,null,null,19403,null,"27_06/05/2021 8:07:19 PM","2021-04-23T23:59:35","Defect","Ship Staff","Ship Staff Insp.","FWD LT cooler sea water Inlet valve Minor seppage through body","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Leak Rectified,","2022-01-22T23:59:35","DLOT220042","Completed","2022-03-09T23:59:35","No","No","No","Internal","valve is ready in Singapore. will be connected to Vsl at next port."]
[null,null,null,18936,null,"27_29/04/2021 5:11:40 PM","2021-04-23T23:59:35","Observation","Ship Staff","Ship Staff Insp.","RUST MARKS AND WEEPS OBSERVED ON THE WINDLASS BRAKE CYLINDER HYDRAULIC CONNECTORS.","Deck - Mooring Machinery","General Appearance","Behaviour Based,External Factors","9.15","Medium","","","Derusting and painiting of Windlass completed","2021-07-23T23:59:35","","Completed","2021-06-24T23:59:35","No","No","No","Internal"]
[null,null,null,18937,null,"27_29/04/2021 5:27:09 PM","2021-04-23T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Exhaudt manifold from ME n DG to SOx Scrubber Insulation cladding rusted and wated at three places.","Miscellaneous","General Appearance","Equipment Related","10.11","Medium","","","Fresh cladding  installed.","2021-07-22T23:59:35","","Completed","2021-05-21T23:59:35","No","No","No","Internal"]
[null,null,null,18939,null,"27_29/04/2021 5:14:10 PM","2021-04-23T23:59:35","Observation","Ship Staff","Ship Staff Insp.","WASTAGE NOTICED DUE TO RUST ON FOAM MONITOR LADDERS FWD OF ACCOMMODATION UNTIL MANIFOLD","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.4","Very High","","","DE-RUSTING/PAINTING CARRIED OUT.","2021-07-23T23:59:35","","Completed","2021-05-07T23:59:35","No","No","No","Internal"]
[null,null,null,16650,null,"27_04/01/2021 4:17:33 PM","2021-04-24T23:59:35","Defect,Observation","Ship Staff","Ship Staff Insp.","SO2 , CO2 , SO2/CO2 RATIO VALUES SHOWING NEGATIVE AND EARACTIC .ALSO SYSTEMS STOPPING AFTER STARTING AGAIN RESTART AFTER SOMETIME STOPS.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.11","Medium","","","S/E attended the V/L on 11th June 12 at Singapore.He replaced the SFU and Cell inlet filter.Cleaned up the contaminated cell mirror with air .Recommended to renew the cell mirror.Now system shows some value of so2/co2 ratio which is quite good at higher ME load .Under observation.SR Engg Attended at Singapore Anchorage as per service rep recommended to renew the Mirror/all Filters/lines cleared and Renewed,Presently SOx/Nox Ratio is Showing,For pending issues will Make new Defect","2021-12-06T23:59:35","","Completed","2022-02-16T23:59:35","No","No","No","Internal"]
[null,null,null,16651,null,"27_04/01/2021 4:36:41 PM","2021-04-24T23:59:35","Breakdown,Defect","Ship Staff","Ship Staff Insp.","BOILER NO.1 DOSING PUMP MOTOR FOUND TO BE HAVING VERY LOW WINDING RESISTANCE. NEED TO ORDER NEW MOTOR.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Spare motor recd and fitted .Dosing pump is operating satisfctory.","2021-07-23T23:59:35","DLOT210024","Completed","2021-06-25T23:59:35","No","No","No","Internal"]
[null,null,null,19404,null,"27_06/05/2021 1:12:16 PM","2021-04-25T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","DG3 FCU booster pump signs of seal leaking","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Leakage observed to be about 10drops in an hour which is normal as suggested by the instruction manual.","2021-05-27T23:59:35","","Completed","2021-05-22T23:59:35","No","No","No","Internal"]
[null,null,null,19405,null,"27_06/05/2021 4:25:06 PM","2021-04-25T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Accommodation Tube light fitting brackets rusted","Deck - Pipe / Fittings","General Appearance","Equipment Related,External Factors","11.1","High","","","De-rusting/Painting of all Accommodation Tubelight brackets completed. Numerous brackets renewed.","2021-08-25T23:59:35","","Completed","2021-08-13T23:59:35","No","No","No","Internal"]
[null,null,null,19406,null,"27_06/05/2021 4:26:58 PM","2021-04-25T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","All SIP vents at various stages of corrossion.","Accommodation,Deck - Pipe / Fittings","General Appearance","Equipment Related","11.6","Medium","","","All SIP vents derusted and painted.","2021-08-25T23:59:35","","Completed","2021-05-03T23:59:35","No","No","No","Internal"]
[null,null,null,19407,null,"27_06/05/2021 4:29:01 PM","2021-04-25T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Accommodation Block and Engine room block casing dirty/spot corrosion evident in China Passage area.","Accommodation","General Appearance","Equipment Related","11.8","Low","","","Derusting and painting of China passage accommodation aft and ER casing fwd bulkhead completed.","2021-08-25T23:59:35"," ","Completed","2021-08-08T23:59:35","No","No","No","Internal"]
[null,null,null,19408,null,"27_06/05/2021 4:31:25 PM","2021-04-25T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Accommodation front Port hole sills rust weeps – spoiling the block paint work.","Accommodation","General Appearance","Equipment Related","11.8","Low","","","Derusting and painting of accommodation front bulkhead completed. Complete cleaning with metal brite carried out.","2021-08-25T23:59:35","","Completed","2021-08-17T23:59:35","No","No","No","Internal"]
[null,null,null,19409,null,"27_06/05/2021 5:09:13 PM","2021-04-25T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ODME unit Vent fan noticed running with high abnormal noise","Deck - Machinery,Miscellaneous","Eng. / Strg. Comp.","Equipment Related","6.13","Low","","","Motor fan cover secured properly and there is no noise now.","2021-08-26T23:59:35","","Completed","2021-06-20T23:59:35","No","No","No","Internal"]
[null,null,null,19410,null,"27_06/05/2021 5:21:34 PM","2021-04-25T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Remote power panel on checking lamps – found few not illuminating","LSA / FFA","Safety / LSA / FFA","Equipment Related","10.11","Medium","","","Fused bulbs replaced","2021-05-26T23:59:35","","Completed","2021-05-17T23:59:35","No","No","No","Internal"]
[null,null,null,19411,null,"27_06/05/2021 5:25:59 PM","2021-04-25T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","EGCS ,Uptake pipe from ER funnel to EGCS tower – insulation cladding fully rusted and wasted on the undersides (at few locations)","Miscellaneous","General Appearance","Equipment Related","10.19","Very High","","","Repaired and renewed the corroded section ","2021-05-25T23:59:35","","Completed","2021-05-20T23:59:35","No","No","No","Internal"]
[null,null,null,19414,null,"27_06/05/2021 5:13:00 PM","2021-04-25T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Old reefr compressor stowed in AHU room ","Miscellaneous","General Appearance","Equipment Related","10.29","Medium","","","Old compressor landed ashore along with the garbage on 11th June 21.","2021-08-25T23:59:35","","Completed","2021-06-06T23:59:35","No","No","No","Internal"]
[null,null,null,19416,null,"27_06/05/2021 1:10:24 PM","2021-04-25T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Eye wash solution seal broken and still kept for use, understand once opened not be used (View ambient temp condition).","Miscellaneous","Eng. / Strg. Comp.","Human Error","8.61","Medium","","","Eye wash replaced","2021-04-26T23:59:35","","Completed","2021-04-26T23:59:35","No","No","No","Internal"]
[null,null,null,19417,null,"27_06/05/2021 1:26:04 PM","2021-04-25T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Singapore Arr Checklist CE sign was missing","Documentation","Crew Management","Human Error","10.3","Medium","","","Corrected","2021-04-25T23:59:35","","Completed","2021-04-25T23:59:35","No","No","No","Internal"]
[null,null,null,19418,null,"27_06/05/2021 1:27:44 PM","2021-04-25T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Night order book – no instructions since 15th April (last seen of at Qingdao)","Documentation","Crew Management","Human Error","","","","","Completed","2021-04-25T23:59:35","","Completed","2021-04-25T23:59:35","No","No","No","Internal"]
[null,null,null,19419,null,"27_06/05/2021 5:27:37 PM","2021-04-25T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Incinerator Flue gas fan lagging/insulation ful of carbon/dirt","Miscellaneous","General Appearance","Equipment Related","10.19","Very High","","","Cleaned and painted.","2021-05-25T23:59:35","","Completed","2021-05-05T23:59:35","No","No","No","Internal"]
[null,null,null,19420,null,"27_06/05/2021 5:16:44 PM","2021-04-25T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","AHU room Ceiling looks dull/dirty at few places","Accommodation","General Appearance","Equipment Related","10.29","Medium","","","Clean and pained","2021-06-26T23:59:35","","Completed","2021-05-04T23:59:35","No","No","No","Internal"]
[null,null,null,19421,null,"27_06/05/2021 5:11:16 PM","2021-04-25T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Elevator Cage floor dirty ","Elect. Mach. & Equip.","General Appearance","Equipment Related","11.17","Low","","","Elevator cage cleaned","2021-05-10T23:59:35","","Completed","2021-05-05T23:59:35","No","No","No","Internal"]
[null,null,null,19422,null,"27_06/05/2021 1:14:28 PM","2021-04-25T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Engine room Most of the bulk heads still dirty  - since DD","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Bulheads  cleaned as required","2021-06-25T23:59:35","","Completed","2021-05-06T23:59:35","No","No","No","Internal"]
[null,null,null,19423,null,"27_06/05/2021 1:29:24 PM","2021-04-25T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Air leaking noise observed from pipe lines above condenser – behind feed water tank in ECR deck","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Air leakage rectified.","2021-05-26T23:59:35","","Completed","2021-05-06T23:59:35","No","No","No","Internal"]
[null,null,null,19424,null,"27_06/05/2021 1:53:36 PM","2021-04-25T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Purifier room Fire door not closing – lock mechanism loose ","E/R - Purifier","Eng. / Strg. Comp.","Equipment Related","5.35","Medium","","","Door closer repaired","2021-05-26T23:59:35","","Completed","2021-05-05T23:59:35","No","No","No","Internal"]
[null,null,null,19425,null,"27_06/05/2021 1:23:10 PM","2021-04-25T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ECR Floor linoleum found dirty/stained","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","ECR Floor cleaned properly","2021-05-20T23:59:35","","Completed","2021-05-05T23:59:35","No","No","No","Internal"]
[null,null,null,19426,null,"27_06/05/2021 1:31:20 PM","2021-04-25T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Service air line valve leaking in purifier room","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Leakage rectified.","2021-05-02T23:59:35","","Completed","2021-05-04T23:59:35","No","No","No","Internal"]
[null,null,null,19427,null,"27_06/05/2021 5:29:55 PM","2021-04-25T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Main engine turbocharger  Suction casing filter cover found chocked","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.12","Very High","",""," CRF raised and approved by office.","2021-05-10T23:59:35","","Completed","2021-05-09T23:59:35","No","No","No","Internal"]
[null,null,null,19428,null,"27_06/05/2021 1:16:48 PM","2021-04-25T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Aft mooring winch Service tank Observed Hyd oil level maintained at min leve","E/R - Aux. Mach.","Eng. / Strg. Comp.","Human Error","9.14","Medium","","","Oil topped up to normal level.","2021-05-02T23:59:35","","Completed","2021-05-08T23:59:35","No","No","No","Internal"]
[null,null,null,19412,null,"27_06/05/2021 8:10:20 PM","2021-04-26T23:59:35","Defect","Ship Staff","Ship Staff Insp.","ME engine flowmwter bypass valve not opening fully when flowmeter is isoalted to meet the fuel cons requirement","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Bypass valve renewed","2021-07-25T23:59:35","","Completed","2021-05-11T23:59:35","No","No","No","Internal"]
[null,null,null,19429,null,"27_13/05/2021 6:28:31 PM","2021-05-03T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Refer rooms temps going up due to gas leakage","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.3","Medium","","","Gas leakage identified at the meat room evaporator 2no.coil bends,same rectified.15kgs of gas charged to the system and observed all temp.normal","2021-08-02T23:59:35","","Completed","2021-05-05T23:59:35","No","No","No","Internal"]
[null,null,null,19430,null,"27_13/05/2021 6:31:44 PM","2021-05-03T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Main sea water pump no.1 mech.seal leaking","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Mech.seal reneweed.","2021-08-02T23:59:35","","Completed","2021-05-07T23:59:35","No","No","No","Internal"]
[null,null,null,19557,null,"27_24/05/2021 10:28:17 AM","2021-05-04T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Deck seal pump no.1 mech.seal leaking and not building pressue.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Pump o;hauled with new seal,shaft,sleeve and mouth rings.","2021-08-04T23:59:35","","Completed","2021-05-17T23:59:35","No","No","No","Internal"]
[null,null,null,19431,null,"27_15/05/2021 2:08:21 PM","2021-05-08T23:59:35","Defect","Ship Staff","Ship Staff Insp.","EGCS Sea water cooling pump no.1 stub pipe adjoining the pump after the suc.valve pin holed and inlet flange weld seam corroded.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.3","Medium","","","Flange section pipe connected to the pump body  renewed and pin hole repaired by putting insert of 100 x100mm.Pipe cleaned thoroughly and 2coats of epoxy applied. ","2021-08-07T23:59:35","","Completed","2021-05-10T23:59:35","No","No","No","Internal"]
[null,null,null,19413,null,"27_16/05/2021 3:23:34 PM","2021-05-09T23:59:35","Critical Equipment","Ship Staff","Ship Staff Insp.","DG3 ACB not closing at times.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.3","Medium","","","Terasaki service engineer attended the V/L on 11th june at Singapore.Checked the tighness of the securing bolts and lubricate the various linkages of the ACB.Currently not facing any problem,hence,closing out.","2021-08-08T23:59:35","","Completed","2021-06-25T23:59:35","No","No","No","Internal"]
[null,null,null,19558,null,"27_21/05/2021 11:09:46 PM","2021-05-13T23:59:35","Critical Equipment","Ship Staff","Ship Staff Insp.","Aux.engine no.2 emergency stop alarm activated on AMS but no alarm indication on the local panel.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","On investigation fault traced with ESB20-Electronic unit engine  safety module.Same renewed .","2021-05-26T23:59:35","","Completed","2021-05-15T23:59:35","No","No","No","Internal"]
[null,null,null,19559,null,"27_21/05/2021 11:14:17 PM","2021-05-15T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Main engine T/C No.2 exh.outlet temp sensor defective alarm activated","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Sensor replaced","2021-08-14T23:59:35","","Completed","2021-05-15T23:59:35","No","No","No","Internal"]
[null,null,null,19560,null,"27_28/05/2021 9:26:36 AM","2021-05-22T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Ref.compressor no.1 mech seal leaking","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Seal renewed.","2021-05-22T23:59:35","","Completed","2021-05-22T23:59:35","No","No","No","Internal"]
[null,null,null,19555,null,"27_31/05/2021 11:53:35 AM","2021-05-25T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Aux.engine no.1 centrifugal filter body found cracked.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.3","Medium","","","Body replaced with  new one.","2021-11-25T23:59:35","DLOT210128","Completed","2021-10-24T23:59:35","No","No","No","Internal"]
[null,null,null,19556,null,"27_31/05/2021 11:58:10 AM","2021-05-25T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Main engine lube oil sump tank low level alarm continuously activating.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Level switch renewed.","2021-08-25T23:59:35","RO DLOT210127","Completed","2021-08-16T23:59:35","No","No","No","Internal"]
[null,null,null,19666,null,"27_09/06/2021 9:21:51 AM","2021-05-27T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Pumproom davit slewing gearbox support cracked and gearbox seized","Deck - Machinery","Safety / LSA / FFA","Equipment Related","5.2","Very High","","","Support weld repaired. Gearbox overhauled. Bearings renewed,  and davit tested.","2021-12-26T23:59:35","DLOT210206","Completed","2022-01-13T23:59:35","No","No","No","Internal","Spares are supplied in the month of Oct 2021. Please check and close the item."]
[null,null,null,17446,null,"27_15/01/2021 11:01:11 PM","2021-06-06T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","RUST WEEP STAINS ON THE ACCOMMODATION FRONT","Accommodation","General Appearance","Behaviour Based","11.8","Low","","","Accommodation front derusted and painted. Full front bulkhead cleaning carried out with metal brite.","2021-09-06T23:59:35","","Completed","2021-08-17T23:59:35","No","No","No","Internal"]
[null,null,null,19852,null,"27_15/06/2021 9:06:52 PM","2021-06-06T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Pipe stach under supports fwd of manifold upto COT #2 – rust weepings","Deck - Pipe / Fittings","General Appearance","External Factors","11.4","Very High","","","Completed piplines till midship. ","2021-12-25T23:59:35","","Completed","2021-12-13T23:59:35","No","No","No","Internal"]
[null,null,null,19853,null,"27_15/06/2021 9:14:37 PM","2021-06-06T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Side Morring winches – looks rusty and rust weepings all over","Deck - Mooring Machinery","Mooring","External Factors","9.14","Medium","","","All windlass and mooring winches derusting and painting completed","2021-07-26T23:59:35","","Completed","2021-07-10T23:59:35","No","No","No","Internal"]
[null,null,null,19854,null,"27_15/06/2021 9:23:56 PM","2021-06-06T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Lot of spot rusts / scattered all over on main deck","Hull & Tanks","General Appearance","External Factors","11.3","Medium","",""," Vessel has completed spot derusting and painting fwd of manifold. Aft of manifold port side till gangway fwd. In progress on stbd side aft of manifold","2021-09-25T23:59:35","","Completed","2021-09-05T23:59:35","No","No","No","Internal"]
[null,null,null,19855,null,"27_15/06/2021 9:50:41 PM","2021-06-06T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Ship Staff Insp.","Draft gauges reported not showing correct readings","Elect. Mach. & Equip.","Cargo / Ballast Systems","External Factors","8.12","Medium","","","Spare zener barrier received and there is no earth fault now.Requires the attendence of the service engineer during V/Ls next call Singapore.","2022-01-26T23:59:35","RO DLOT210163 Raised","Completed","2022-01-11T23:59:35","No","No","No","Internal"]
[null,null,null,19856,null,"27_15/06/2021 9:54:06 PM","2021-06-06T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Ship Staff Insp.","Cable supports on deck – at various stages of corrosion/wastage","Deck - Pipe / Fittings","General Appearance","External Factors","","","","","Derusted and painted – Ensured proper surface prepartion prior final coat. ","2021-12-25T23:59:35","","Completed","2022-01-07T23:59:35","No","No","No","Internal"]
[null,null,null,19857,null,"27_15/06/2021 9:58:46 PM","2021-06-06T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","WBT Vent flanges were rusty","Deck - Pipe / Fittings","Cargo / Ballast Systems","External Factors","11.7","High","","","Completed derusting and painting of all WBT vents on main deck.","2021-08-26T23:59:35","","Completed","2021-08-13T23:59:35","No","No","No","Internal"]
[null,null,null,19858,null,"27_15/06/2021 10:08:04 PM","2021-06-06T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","All butterworth covers, manhole doors flanges rusty","Hull & Tanks","Cargo / Ballast Systems","External Factors","","","","","All manhole covers onboard derusted and painting completed","2021-12-15T23:59:35","","Completed","2021-11-12T23:59:35","No","No","No","Internal"]
[null,null,null,19859,null,"27_15/06/2021 10:10:29 PM","2021-06-06T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Aft of accommodation block in china passage lot of areas (scattered) under various stages of corrosion/rust weepings","Accommodation","General Appearance","External Factors","11.8","Low","","","Completed derusting and full coat painting of China passage Accommodation and ER bulkheads.","2021-09-06T23:59:35","","Completed","2021-08-08T23:59:35","No","No","No","Internal"]
[null,null,null,19860,null,"27_15/06/2021 10:12:17 PM","2021-06-06T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Ship Staff Insp.","Aft of casing in poop deck - lot of areas (scattered) under various stages of corrosion/rust weepings","Accommodation","General Appearance","External Factors","11.8","Low","","","Completed derusting and painting of bulkheads aft of poop deck and full coat painting.","2021-09-06T23:59:35","","Completed","2021-07-31T23:59:35","No","No","No","Internal"]
[null,null,null,19861,null,"27_16/06/2021 11:24:49 AM","2021-06-06T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Ship Staff Insp.","Main engine fuel pumps bottom spaces inspection windows kept open permanently","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.2","Low","","","Covers fabricated.","2021-07-16T23:59:35","","Completed","2021-07-12T23:59:35","No","No","No","Internal"]
[null,null,null,19862,null,"27_16/06/2021 1:04:48 PM","2021-06-06T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Waste oil drums near incinerator platform found collected with sludge and soot ","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","6.16","Very High","","","Sludge and soot  cleared","2021-07-21T23:59:35","","Completed","2021-07-05T23:59:35","No","No","No","Internal"]
[null,null,null,19863,null,"27_16/06/2021 1:08:28 PM","2021-06-06T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","EGCS CEMS Unit-Maker SE advised ambient temp high and hence sensor trouble.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.11","Medium","","","RO Raised by the office for the cooling unit.","2021-08-06T23:59:35","RO DLOT215038","Completed","2021-07-08T23:59:35","No","No","No","Internal"]
[null,null,null,19864,null,"27_18/06/2021 2:03:57 PM","2021-06-06T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Gangway Air line filters moisture drain not working ","Deck - Machinery","Safety / LSA / FFA","Human Error","5.47","Medium","","","Gangway air filter lubricators replaced with new ones.","2021-09-10T23:59:35","","Completed","2021-08-16T23:59:35","No","No","No","Internal"]
[null,null,null,19866,null,"27_16/06/2021 1:13:53 PM","2021-06-06T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","FWG Ejector pump discharge valve leaking from the body.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","RO Raised.","2021-08-06T23:59:35","DLOT210131","Completed","2021-06-10T23:59:35","No","No","No","Internal"]
[null,null,null,19867,null,"27_16/06/2021 1:10:49 PM","2021-06-06T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","AE3 shall fall due for cyl.head overhaul","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","RO Raised.","2021-07-06T23:59:35","RO DLOT210142","Completed","2021-06-10T23:59:35","No","No","No","Internal"]
[null,null,null,19868,null,"27_16/06/2021 11:13:18 AM","2021-06-06T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Ship Staff Insp.","Vaccum condenser sea water inlet,outlet lines connected to condenser-salt deposits in flanges.","E/R - Pipes/ valves & fittings","Emgcy. Systems","Equipment Related","10.31","Very High","","","Flanges tightened and leakage rectified.","2021-08-06T23:59:35","","Completed","2021-06-12T23:59:35","No","No","No","Internal"]
[null,null,null,19869,null,"27_16/06/2021 10:24:59 AM","2021-06-06T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","LT Cooler sea water leaking from vent connection","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.31","Very High","","","Leakage rectified","2021-06-27T23:59:35","","Completed","2021-06-12T23:59:35","No","No","No","Internal"]
[null,null,null,19870,null,"27_18/06/2021 11:39:31 AM","2021-06-06T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Stbd hose crane hositing winch gear box oil level low","Deck - Machinery","Cargo / Ballast Systems","Human Error","8.5","Very High","","","Gear oil checked and refilled.","2021-06-21T23:59:35","DLOT210137","Completed","2021-06-12T23:59:35","No","No","No","Internal"]
[null,null,null,19871,null,"27_18/06/2021 11:41:38 AM","2021-06-06T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Both provision cranes hoisting winch gear box oil level low","Deck - Machinery","Cargo / Ballast Systems","Human Error","8.5","Very High","","","Checked and refilled.","2021-06-21T23:59:35","","Completed","2021-06-12T23:59:35","No","No","No","Internal"]
[null,null,null,19872,null,"27_18/06/2021 12:04:43 PM","2021-06-06T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Ship Staff Insp.","Both dryer filters found fully chocked","Accommodation","Safety / LSA / FFA","Human Error","11.14","Medium","","","Both dryers filters cleaned and to be regularly inspected in future","2021-06-12T23:59:35","","Completed","2021-06-07T23:59:35","No","No","No","Internal"]
[null,null,null,19873,null,"27_16/06/2021 12:55:27 PM","2021-06-06T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","EGCS Scrubber wash water pipe from tower in poop deck ,pipe bottom support beam bolt rusted heavily.","Deck - Pipe / Fittings","General Appearance","Equipment Related","10.11","Medium","","","Bolts replaced with SS.","2021-08-06T23:59:35","","Completed","2021-06-13T23:59:35","No","No","No","Internal"]
[null,null,null,19874,null,"27_16/06/2021 09:20:58","2021-06-06T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Elevator floor fully stained and dirty.","Miscellaneous","General Appearance","Equipment Related","11.8","Low","","","Cleaned and mat put on the floor.","2021-06-27T23:59:35","","Completed","2021-06-15T23:59:35","No","No","No","Internal"]
[null,null,null,19875,null,"27_16/06/2021 11:28:25 AM","2021-06-06T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Air line leaking noise near EGCS sea water pump","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","11.4","Very High","","","Leakage rectified.","2021-06-16T23:59:35","","Completed","2021-06-14T23:59:35","No","No","No","Internal"]
[null,null,null,19876,null,"27_16/06/2021 11:33:08 AM","2021-06-06T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Instrument air/control air is being supplied from service air compressor","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related","11.4","Very High","","","Service air compressor dedicated for the control air.","2021-06-21T23:59:35","","Completed","2021-06-13T23:59:35","No","No","No","Internal"]
[null,null,null,19877,null,"27_16/06/2021 11:37:48 AM","2021-06-06T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","WEMS pump cabinet door noticed kept open and external cooling fan provided.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.37","Medium","","","As a precautionary measure,cabinet kept open to prevent overheating of the bottle.However,small supply fan is provided in the cabinet by makers.","2021-07-06T23:59:35","","Completed","2021-06-14T23:59:35","No","No","No","Internal"]
[null,null,null,19878,null,"27_16/06/2021 12:42:18 PM","2021-06-06T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","No separate air bottle for control air -as same is being supplied directly.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","RO Raised for the deck service air compressor.","2021-09-06T23:59:35","RO DLOT210145","Completed","2021-06-15T23:59:35","No","No","No","Internal"]
[null,null,null,19879,null,"27_16/06/2021 12:50:29 PM","2021-06-06T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Both Aux.boilers remote operating cables for gauge cocks and valves found seized.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Release gears eased up and stenciled properly. ","2021-06-21T23:59:35","","Completed","2021-06-17T23:59:35","No","No","No","Internal"]
[null,null,null,19880,null,"27_15/06/2021 9:44:15 PM","2021-06-06T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Ship Staff Insp.","Stbd side MARPOL line – valve reported not holding","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.11","Medium","","","Valve opened and repaired. Seat ring renewed.","2021-07-21T23:59:35","","Completed","2021-06-11T23:59:35","No","No","No","Internal"]
[null,null,null,19881,null,"27_16/06/2021 09:16:44","2021-06-06T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Ship Staff Insp.","Purifier room switchboard dirty","Elect. Mach. & Equip.","General Appearance","Equipment Related","11.1","High","","","All panels wiped/cleaned properly.","2021-07-06T23:59:35","","Completed","2021-06-16T23:59:35","No","No","No","Internal"]
[null,null,null,19882,null,"27_15/06/2021 9:40:48 PM","2021-06-06T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","VRC valve boxes on deck.Noticed silica gel packs missing – to avoid moisture","Cargo Mach.","Cargo / Ballast Systems","Human Error","8.11","Medium","","","Silica gel packs kept inside the VRC valve boxes.","2021-07-06T23:59:35","","Completed","2021-06-17T23:59:35","No","No","No","Internal"]
[null,null,null,19883,null,"27_16/06/2021 09:12:20","2021-06-06T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","E/R Workshop  bulk heads dirty,floor needs full coat of paint","Miscellaneous","General Appearance","Equipment Related","10.3","Medium","","","W/Shop bulkheads water washed /cleaned.","2021-07-06T23:59:35","","Completed","2021-06-19T23:59:35","No","No","No","Internal"]
[null,null,null,19884,null,"27_16/06/2021 12:59:54 PM","2021-06-06T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Sealing air line to uptake damper-position switch air line leaking (EGB deck)","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","To trace and rectify the leakage.","2021-07-06T23:59:35","","Completed","2021-06-21T23:59:35","No","No","No","Internal"]
[null,null,null,19885,null,"27_16/06/2021 12:37:34 PM","2021-06-06T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Hyper mist system sensors above AE2 and AE3 not working","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.18","High","","","AE3 sensor replced with a spare one and AE2 is functioning satisfactory as the E/R temp .is low at present.Will modify the air trunking towards AE2 sensor in order to avoid sensor activation at higher E/R room.","2021-07-06T23:59:35","","Completed","2021-06-22T23:59:35","No","No","No","Internal"]
[null,null,null,19886,null,"27_15/06/2021 10:22:20 PM","2021-06-06T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Air line filters moisture drain not working ","Deck - Machinery","Safety / LSA / FFA","Equipment Related","5.47","Medium","","","DDRL already created","2021-06-06T23:59:35","","Completed","2021-06-06T23:59:35","No","No","No","Internal"]
[null,null,null,19887,null,"27_15/06/2021 9:17:55 PM","2021-06-06T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Windlass Equipment in whole Looks rusty ","Deck - Mooring Machinery","Mooring","External Factors","9.14","Medium","","","Derusting and painting completed. ","2021-07-10T23:59:35","","Completed","2021-07-25T23:59:35","No","No","No","Internal"]
[null,null,null,19888,null,"27_01/07/2021 2:11:27 PM","2021-06-06T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ER tube lights-Noticed the fittings had mix of Fluorescent and LED tube lights.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.3","Medium","","","Mixed of Fluorescent and LED tube lights has been sorted out.","2021-08-06T23:59:35","","Completed","2021-06-20T23:59:35","No","No","No","Internal"]
[null,null,null,19667,null,"27_14/06/2021 19:20:59","2021-06-07T23:59:35","Defect","Ship Staff","Ship Staff Insp.","AE1 and A/E2 No.1 Fuel oil booster pump mech seal leaking","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Mech seal renewed.","2021-09-07T23:59:35","","Completed","2021-06-09T23:59:35","No","No","No","Internal"]
[null,null,null,19865,null,"27_01/07/2021 1:19:26 PM","2021-06-16T23:59:35","Defect","Ship Staff","Ship Staff Insp.","EGCS Sea water cooling pump no.1 VFD Inverter cooling fan making abnormal noise and activating alarm","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Fan to be replced.","2021-10-16T23:59:35","RO DLOT210149","Completed","2021-10-22T23:59:35","No","No","No","Internal"]
[null,null,null,20035,null,"27_15/07/2021 13:53:53","2021-06-27T23:59:35","Defect","Ship Staff","Ship Staff Insp.","OWS Feed pump body/shaft badly corroded","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Pump temporarily repaired and awaiting for the complete pump renewal.","2021-12-26T23:59:35","RO DLOT210150","Completed","2022-02-22T23:59:35","No","No","No","Internal","Awaiting readiness from Japan. Makers have long supply time."]
[null,null,null,20036,null,"27_05/07/2021 8:27:08 PM","2021-06-29T23:59:35","Defect","Ship Staff","Ship Staff Insp.","EGCS Sea water cooling pump no.2 stub pipe  after the suc.valve corroded/holed.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.3","Medium","","","Pipe section adjoining the pump body  renewed and other side of the stub pipe not renewed.2-Coats of epoxy applied and fitted in place.","2021-09-29T23:59:35","","Completed","2021-07-03T23:59:35","No","No","No","Internal"]
[null,null,null,20037,null,"27_05/07/2021 8:29:47 PM","2021-06-30T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Deck seal pump no.2 stub piece before the discharge valve holed","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.3","Medium","","","Stub piece renewed","2021-09-29T23:59:35","","Completed","2021-07-04T23:59:35","No","No","No","Internal"]
[null,null,null,20038,null,"27_10/07/2021 23:53:29","2021-06-30T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Main engine lube oil pump no.1 motor bearing coupling side making abnormal sound.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","","","","","Motor over hauled","2021-09-29T23:59:35","","Completed","2021-07-05T23:59:35","No","No","No","Internal"]
[null,null,null,20203,null,"27_19/07/2021 8:35:37 PM","2021-07-11T23:59:35","Defect","Ship Staff","Ship Staff Insp.","ME RPLS Pumps relief valve leaking","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Dismantled and o-ring renewed.","2021-10-10T23:59:35","","Completed","2021-07-14T23:59:35","No","No","No","Internal"]
[null,null,null,20208,null,"27_19/07/2021 8:30:24 PM","2021-07-11T23:59:35","Defect","Ship Staff","Suptd. Insp.","HP soot blowers air line holed/corroded after the main sol.operated valve.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Pipe section of L3100mm x NB 80 mm corroded section renewed","2021-10-10T23:59:35","","Completed","2021-07-15T23:59:35","No","No","No","Internal"]
[null,null,null,20204,null,"27_22/07/2021 3:49:49 PM","2021-07-13T23:59:35","Defect","Ship Staff","Ship Staff Insp.","FWG Heat exchanger JCW FW inlet and outlet valve passing","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Valves replaced with the new ones.","2021-10-13T23:59:35","","Completed","2021-07-14T23:59:35","No","No","No","Internal"]
[null,null,null,22358,null,"27_22/10/2021 2:36:14 PM","2021-07-14T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Cargo Audit","MSDS was not discussed among crew members in pre meeting. No records have been found in the port logbook.","Documentation","Safety / LSA / FFA","Human Error","5.46","Medium","","","Entry made in CCR logbooks in pre arrival loading meeting mentioning MSDS of cargoes discussed.","2021-08-14T23:59:35","","Completed","2021-07-15T23:59:35","No","No","No","Internal"]
[null,null,null,20205,null,"27_29/07/2021 9:24:01 PM","2021-07-21T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Fire and GS Pump mechanical seal leaking.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Motor removed from place and pump dismantled.Mech.seal lapped as having no spare and boxed back.Currently there is no leak.","2021-10-20T23:59:35","","Completed","2021-07-22T23:59:35","No","No","No","Internal"]
[null,null,null,20206,null,"27_29/07/2021 9:30:25 PM","2021-07-23T23:59:35","Defect","Ship Staff","Ship Staff Insp.","AE2 T/C making abnormal noise.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","AE2 Isolated and T/C dismantled.Removed cartridge having play in the bearing which caused the rubbing of the blower and turbine impeller with the housing.","2021-10-22T23:59:35","","Completed","2021-07-24T23:59:35","No","No","No","Internal"]
[null,null,null,20207,null,"27_29/07/2021 9:40:01 PM","2021-07-23T23:59:35","Defect","Ship Staff","Ship Staff Insp.","AE2 T/C giving abnormal noise.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","AE2 Isolated and T/C dismantled.On investigation ,it was observed that there is play in the bearings which caused the T/C blower as well turbine impleller to rub slightly with the casing.T/C boxed back with re-conditined cartridge and old good nozzle ring-all to be in order","2021-10-22T23:59:35","","Completed","2021-07-24T23:59:35","No","No","No","Internal"]
[null,null,null,20202,null,"27_01/08/2021 13:58:19","2021-07-24T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Aft hyd.system for the mooring winches inlet line flange leaking from the o-ring close to the steering gear compartment bulkhead.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Flange o-ring needs to be renewed.","2021-10-23T23:59:35","","Completed","2021-07-28T23:59:35","No","No","No","Internal"]
[null,null,null,20362,null,"27_15/08/2021 16:11:29","2021-07-28T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Fire and GS pump priming pump tank corroded/holed","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Priming tank renewed","2021-10-28T23:59:35","","Completed","2021-07-30T23:59:35","No","No","No","Internal"]
[null,null,null,20363,null,"27_15/08/2021 16:15:34","2021-07-30T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Bilge,Fire and Ballast pump priming pump tank corroded/holed","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Priming tank fabricated and fitted in place.","2021-07-30T23:59:35","","Completed","2021-08-02T23:59:35","No","No","No","Internal"]
[null,null,null,20364,null,"27_15/08/2021 16:35:19","2021-08-03T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Hyd.leak from Port windlass brake cylinder","Deck - Mooring Machinery","Mooring","Equipment Related","9.2","Very High","","","Leakage rectified by renewing the seal.","2021-08-03T23:59:35","","Completed","2021-08-03T23:59:35","No","No","No","Internal"]
[null,null,null,20367,null,"27_15/08/2021 16:21:09","2021-08-04T23:59:35","Defect","Ship Staff","Ship Staff Insp.","HFO Transfer pump mech.seal passing","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Pump overhauled and boxed back with new bearings ,mech.seal.","2021-08-04T23:59:35","","Completed","2021-08-05T23:59:35","No","No","No","Internal"]
[null,null,null,20365,null,"27_15/08/2021 16:30:45","2021-08-05T23:59:35","Defect","Ship Staff","Ship Staff Insp.","HFO.Purifier no.1 fuel oil feed pump mech.seal passing","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","","","","","Pump overhauled.","2021-08-05T23:59:35","","Completed","2021-08-05T23:59:35","No","No","No","Internal"]
[null,null,null,20366,null,"27_15/08/2021 16:25:15","2021-08-06T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Main engine fuel oil supply pump no.1 making abnormal noise.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Pump overhauled and working satisfactory","2021-08-06T23:59:35","","Completed","2021-08-06T23:59:35","No","No","No","Internal"]
[null,null,null,20685,null,"27_21/08/2021 18:11:18","2021-08-12T23:59:35","Defect","Ship Staff","Ship Staff Insp.","FWG Ejector pump motor making abmormal noise.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Motor overhauled and coupling bushes renewed","2021-11-12T23:59:35","","Completed","2021-08-14T23:59:35","No","No","No","Internal"]
[null,null,null,20686,null,"27_21/08/2021 18:13:49","2021-08-16T23:59:35","Defect","Ship Staff","Ship Staff Insp.","M/E Unit no.5 exh.high temp alarm activated","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Fault traced with the sensor,same renewed","2021-11-15T23:59:35","","Completed","2021-08-16T23:59:35","No","No","No","Internal"]
[null,null,null,22359,null,"27_25/10/2021 9:32:18 AM","2021-08-21T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Stbd side No2 Manifold valve seat ring found damaged and leaking.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.41","Medium","","","Damaged seat ring renewed.","2021-09-21T23:59:35","","Completed","2021-09-05T23:59:35","No","No","No","Internal"]
[null,null,null,20687,null,"27_01/09/2021 11:12:05 AM","2021-08-21T23:59:35","Defect","Ship Staff","Ship Staff Insp.","M/E Fuel oil booster pump no.1 giving abnormal vibration","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Pump overhauled with new bearings and mech.seal","2021-11-20T23:59:35","","Completed","2021-08-25T23:59:35","No","No","No","Internal"]
[null,null,null,22360,null,"27_25/10/2021 9:26:20 AM","2021-08-22T23:59:35","Observation","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","The Engine room night order book was written by CE on 26th Aug 2021, however it was signed by 4/E only.","Documentation","Eng. / Strg. Comp.","Human Error","","","","","The standing orders were signed. Training carried out for all officers. Standing orders promptly signed.","2021-09-21T23:59:35","","Completed","2021-08-23T23:59:35","No","No","No","External"]
[null,null,null,22361,null,"27_25/10/2021 9:18:26 AM","2021-08-22T23:59:35","Observation","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","The Master and chief officer joined the vessel on 8th May 2021 and offsigners(master/CO) disembarked on 8th May 2021. Master and CO did not have such vessel experiance.","Documentation","Cert. & Docu.","External Factors","3.5","Medium","","","COVID-19 restrictions at vessel's port of call and unavailablity of flights has severly impacted crew reliefs making it impossible to stagger reliefs.","2021-09-22T23:59:35","","Completed","2021-09-02T23:59:35","No","No","No","External"]
[null,null,null,20974,null,"27_19/09/2021 2:14:15 PM","2021-08-24T23:59:35","Defect","Ship Staff","Ship Staff Insp.","No.1 STBD manifold valve found leaking","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.11","Medium","","","Inspection found damaged seat ring, same renewed, Bolts renewed.","2021-09-28T23:59:35","","Completed","2021-08-29T23:59:35","No","No","No","Internal"]
[null,null,null,22362,null,"27_25/10/2021 2:43:39 PM","2021-08-30T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Fire nozzle securing clamp in the fire box found out of order. Location – Port bridge wing.","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.38","High","","","The securing clamp was fixed and now in order.","2021-11-29T23:59:35","","Completed","2021-08-31T23:59:35","No","No","No","Internal"]
[null,null,null,22363,null,"27_25/10/2021 2:46:41 PM","2021-08-30T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Forward mast head securing wires (wire stays) found to be dried-up, which need to be lubricated. ","Miscellaneous","General Appearance","External Factors","11.8","Low","","","Securing wires cleaned and greasing carried out.","2021-11-29T23:59:35","","Completed","2021-09-03T23:59:35","No","No","No","Internal"]
[null,null,null,22364,null,"27_25/10/2021 2:51:06 PM","2021-08-30T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Used Eye wash solution with cap opened found at the entrance of Fore peak store. ( 0.9% sterile saline solution is used for irrigating eyes and general wound washing applications)","Miscellaneous","Safety / LSA / FFA","Human Error","5.46","Medium","","","The strile eye wash bottle was replaced with a new bottle","2021-09-29T23:59:35","","Completed","2021-08-31T23:59:35","No","No","No","Internal"]
[null,null,null,22365,null,"27_25/10/2021 2:54:39 PM","2021-08-30T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ODME vent near pump room entrance (stbd side) found badly rusted","Deck - Pipe / Fittings","General Appearance","External Factors","11.7","High","","","ODME vent near pumproom entrance derusted and painted.","2021-10-30T23:59:35","","Completed","2021-09-07T23:59:35","No","No","No","Internal"]
[null,null,null,22366,null,"27_25/10/2021 2:57:34 PM","2021-08-30T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Common laundry room on upper deck needs cleaning","Accommodation","General Appearance","Behaviour Based","11.13","Low","","","Common laundry room on upper deck cleaned and fresh paint applied to deck.","2021-09-29T23:59:35","","Completed","2021-09-09T23:59:35","No","No","No","Internal"]
[null,null,null,22367,null,"27_25/10/2021 3:02:21 PM","2021-08-30T23:59:35","Observation","Owner / Marine / Tech. Suptd.","MLC Audit","Following financial security certificates were not displayed in common areas .\n\n\n\naa) Certificate of Insurance or other financial security in respect of seafarer repatriation costs and liabilities as required under regulation 2.5.2 ,standard A 2.5.2 \n\n\n\nbb) Certificate of Insurance or other financial security in respect of ship owner’s liability  as required under regulation 4.2  \n\n","Documentation","Cert. & Docu.","Human Error","2.1","Very High","","","The required certificate copies displayed in common areas.","2021-09-29T23:59:35","","Completed","2021-08-31T23:59:35","No","No","No","Internal"]
[null,null,null,21351,null,"27_23/09/2021 11:15:36 AM","2021-08-30T23:59:35","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Refer compressor suc/discharge line lagging damaged","E/R - Aux. Mach.","General Appearance","Equipment Related","10.32","Very High","","","Lagging renewed and secured properly","2021-09-29T23:59:35","","Completed","2021-09-29T23:59:35","No","No","No","Internal"]
[null,null,null,21352,null,"27_23/09/2021 11:37:38 AM","2021-08-30T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ER Funnel aft exhaust window for various vents-full of oil steaks and looks very dirty","Miscellaneous","General Appearance","Equipment Related","10.32","Very High","","","cleaned and painted. ","2021-12-25T23:59:35","","Completed","2021-12-06T23:59:35","No","No","No","Internal"]
[null,null,null,21353,null,"27_23/09/2021 12:02:39 PM","2021-08-30T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","EGCS Exh.gas flow sensor HT alarm recurring","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","High temp.alarm recurring due to Booster pump low pressure which is due to  dislodge of the pipe end flange which is repaired by using Nylon-Thistlebond putty.","2021-09-29T23:59:35","","Completed","2021-10-01T23:59:35","No","No","No","Internal"]
[null,null,null,21354,null,"27_23/09/2021 12:05:59 PM","2021-08-30T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","MGPS Anodes are not getting consumed","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","As per Makers advise,MGPS anodes coneections to re- check and to use back up panel.l","2021-12-26T23:59:35","","Completed","2022-01-16T23:59:35","No","No","No","Internal"]
[null,null,null,21355,null,"27_23/09/2021 12:18:32 PM","2021-08-30T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Cargo few lines on deck noticed with rust patches","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.4","Very High","","","Completed derusting and painting.","2021-11-05T23:59:35","","Completed","2021-10-26T23:59:35","No","No","No","Internal"]
[null,null,null,21356,null,"27_23/09/2021 12:22:46 PM","2021-08-30T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Cow lines on deck,Flanges noticed rusty","Deck - Pipe / Fittings","General Appearance","Equipment Related","8.34","High","","","All COW lines on deck derusted and painted.","2021-11-05T23:59:35","","Completed","2021-11-06T23:59:35","No","No","No","Internal"]
[null,null,null,21357,null,"27_23/09/2021 12:25:28 PM","2021-08-30T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","COW machine,Flanges tusty","Deck - Pipe / Fittings","General Appearance","Equipment Related","8.34","High","","","All COW machines and flanges derusted and painted.","2021-11-05T23:59:35","","Completed","2021-11-06T23:59:35","No","No","No","Internal"]
[null,null,null,21358,null,"27_23/09/2021 12:28:09 PM","2021-08-30T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Deck Forward area ,Tank manhole covers /flanges rusted","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.3","Medium","","","Derusting and painting completed.","2021-09-29T23:59:35","","Completed","2021-09-29T23:59:35","No","No","No","Internal"]
[null,null,null,21363,null,"27_23/09/2021 11:49:23 AM","2021-08-30T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","EGCS,on top platform ,temp ropes secured for support to work on CEMS Sensors","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","Suggest to rig railing only on the sensor.We feel, it is more safe to have the rope all around,hence,will keep as it is.","2021-09-29T23:59:35","","Completed","2021-09-18T23:59:35","No","No","No","Internal"]
[null,null,null,21364,null,"27_23/09/2021 11:26:08 AM","2021-08-30T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Gymnasium CPU not lashed","Miscellaneous","General Appearance","Equipment Related","","","","","All items secured","2021-09-29T23:59:35","","Completed","2021-09-18T23:59:35","No","No","No","Internal"]
[null,null,null,21365,null,"27_23/09/2021 12:09:49 PM","2021-08-30T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","EGCS Sea water pumps (both)sea suction elbowswith soft patch","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Drawing has been sent to ofice for fabrication of pipes ashore","2021-09-23T23:59:35","","Completed","2021-09-17T23:59:35","No","No","No","Internal"]
[null,null,null,21366,null,"27_23/09/2021 12:14:55 PM","2021-08-30T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Ship Staff Insp.","Refer rooms frosting observed in refrigerant return line in lobby","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","System checked and observed sufficient gas","2021-09-25T23:59:35","","Completed","2021-09-18T23:59:35","No","No","No","Internal"]
[null,null,null,21367,null,"27_23/09/2021 11:58:55 AM","2021-08-30T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Steering space natural vent frame rusted","Miscellaneous","General Appearance","Equipment Related","","","","","Derusted and painted.","2021-09-29T23:59:35","","Completed","2021-09-22T23:59:35","No","No","No","Internal"]
[null,null,null,21368,null,"27_23/09/2021 11:11:47 AM","2021-08-30T23:59:35","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","AHU Casing exterior dirty","Miscellaneous","General Appearance","Equipment Related","","","","","Casing painted","2021-09-29T23:59:35","","Completed","2021-09-19T23:59:35","No","No","No","Internal"]
[null,null,null,21369,null,"27_23/09/2021 11:55:15 AM","2021-08-30T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","EGCS Foundation support Port aft rusted","Miscellaneous","General Appearance","Equipment Related","10.32","Very High","","","Derusted and painted.","2021-09-29T23:59:35","","Completed","2021-09-22T23:59:35","No","No","No","Internal"]
[null,null,null,21370,null,"27_23/09/2021 11:22:25 AM","2021-08-30T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Laundry room lightig looks not sufficient-not bright enough","Miscellaneous","General Appearance","Equipment Related","10.32","Very High","","","LED Tubes wattage cannot be increased.However,diffusers cleaned up and lighting slightly improved. ","2021-09-29T23:59:35","","Completed","2021-09-20T23:59:35","No","No","No","Internal"]
[null,null,null,21371,null,"27_23/09/2021 11:31:48 AM","2021-08-30T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Fire control station spare UM1 Batteries were kept loose on top of the switchboard","Miscellaneous","General Appearance","Equipment Related","","","","","Ensure batteries stowed properly","2021-09-19T23:59:35","","Completed","2021-09-19T23:59:35","No","No","No","Internal"]
[null,null,null,20973,null,"27_19/09/2021 1:23:45 PM","2021-09-03T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Deck service air In-operational","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Fault traced with Contactors.","2021-12-02T23:59:35","RO DLOT210205 Raised","Completed","2021-10-20T23:59:35","No","No","No","Internal"]
[null,null,null,20975,null,"27_19/09/2021 2:16:56 PM","2021-09-08T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Main air compressor starter panel not diplaying any parameters ","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Fault traced with PLC, same renewed ","2021-12-08T23:59:35","","Completed","2021-09-09T23:59:35","No","No","No","Internal"]
[null,null,null,22368,null,"27_25/10/2021 9:58:36 AM","2021-09-10T23:59:35","Defect","Ship Staff","Ship Staff Insp.","During derusting and painting, bunker drain line found holed.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","6.7","High","","","Line taken to ER room. New section fixed and bunker drain line fixed back.","2021-09-15T23:59:35","","Completed","2021-09-12T23:59:35","No","No","No","Internal"]
[null,null,null,21359,null,"27_21/09/2021 20:44:24","2021-09-16T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Vaccum condenser sea water pipe  pin holed/thinned after the outlet valve.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Temporarily repaired by welding doubler.Prior to the pipe renewal,bypass valve needs to be renewed.Added in REFMAN for DD Jobs","2021-12-16T23:59:35","","Completed","2021-11-10T23:59:35","No","No","No","Internal"]
[null,null,null,21360,null,"27_21/09/2021 20:48:29","2021-09-16T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Vaccum condenser by pass valve passing","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Valve eased up, Presently holding,","2021-12-16T23:59:35","","Completed","2022-01-14T23:59:35","No","No","No","Internal"]
[null,null,null,21361,null,"27_22/09/2021 12:34:23 PM","2021-09-17T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Sea water valve connecting LT coolers and Vaccum condenser seized in open position","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Valve needs to be renewed.Added in REFMAN for DD Jobs","2021-12-17T23:59:35","RO DLOT210131","Completed","2021-11-10T23:59:35","No","No","No","Internal"]
[null,null,null,21362,null,"27_29/09/2021 11:49:13","2021-09-20T23:59:35","Defect","Ship Staff","Ship Staff Insp.","EGCS Booster pump wash pipe end damage","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Maker Technician cropped and renewed the damaged section of piping, Presently no leaks observed and SW Pr Steady at 3.8bar","2021-12-20T23:59:35","","Completed","2021-11-28T23:59:35","No","No","No","Internal"]
[null,null,null,22369,null,"27_25/10/2021 10:17:17 AM","2021-09-25T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Stbd manifold common cargo drain line to 3S COT was found holed.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.41","Medium","","","The damaged section was removed and taken to ER workshop. Welding repairs carried out and line fixed back.","2021-10-05T23:59:35","","Completed","2021-09-28T23:59:35","No","No","No","Internal"]
[null,null,null,21585,null,"27_14/10/2021 5:51:29 PM","2021-09-27T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Economiser wash drain valve seized in open position","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Valve overhauled","2021-09-27T23:59:35","","Completed","2021-09-30T23:59:35","No","No","No","Internal"]
[null,null,null,21583,null,"27_14/10/2021 5:55:48 PM","2021-10-06T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Main engine slowed down due to oil mist high alarm of gear case.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Oil mist detector renewed.","2021-10-06T23:59:35","","Completed","2021-10-06T23:59:35","No","No","No","Internal"]
[null,null,null,21584,null,"27_14/10/2021 6:00:41 PM","2021-10-06T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Harbour sea water pump motor making abnormal noise and pump mech.seal passing.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Motor and Pump overhauled.Pump boxed back with new line bearing,wear rings and Mech.seal.Motor both bearings renewed.","2021-12-05T23:59:35","","Completed","2021-10-09T23:59:35","No","No","No","Internal"]
[null,null,null,21582,null,"27_14/10/2021 6:04:04 PM","2021-10-08T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Sewage plant air compressor tripped on overload.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Compressor overhauled","2021-12-08T23:59:35","","Completed","2021-10-25T23:59:35","No","No","No","Internal"]
[null,null,null,22370,null,"27_18/10/2021 3:36:14 PM","2021-10-13T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Main air compressor no.2 soft starter mal-functioning","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Soft starter needs to be renewed.","2021-12-12T23:59:35","DLOT RO210140","Completed","2021-10-25T23:59:35","No","No","No","Internal"]
[null,null,null,22371,null,"27_25/10/2021 7:01:22 AM","2021-10-19T23:59:35","Defect","Ship Staff","Ship Staff Insp.","ME Unit no.2 exh.high temp.alarm activated and followed by T/C high temp caused ME slow down","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Problem traced with the spill valve push rod and umbrela seal,same renewed.","2021-10-19T23:59:35","","Completed","2021-10-19T23:59:35","No","No","No","Internal"]
[null,null,null,22709,null,"27_03/11/2021 7:35:14 AM","2021-10-28T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Railings on deck and outside accommodation found damaged. Total 17 locations identified","Deck - Pipe / Fittings","General Appearance","External Factors","11.3","Medium","","","temporary repairs carried out, and need to do hot work. same entered into REFMAN","2022-01-26T23:59:35","","Completed","2022-01-17T23:59:35","No","No","No","Internal","Please plan and complete the job ASAP."]
[null,null,null,22710,null,"27_03/11/2021 10:08:47 AM","2021-10-28T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Main sea water pump no.1 sea suction valve body holed/wasted","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Valve needs to be renewed,Added in REFMAN For DD Jobs,","2022-01-28T23:59:35","DLOT220088","Completed","2021-11-10T23:59:35","No","No","No","Internal"]
[null,null,null,22711,null,"27_05/11/2021 6:08:24 AM","2021-10-29T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Fire & GS Pump mech.seal slightly leaking","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Mech.sea and shaft seal renewed and all in order.","2022-01-29T23:59:35","RO DLOT 210177","Completed","2021-11-05T23:59:35","No","No","No","Internal"]
[null,null,null,23046,null,"27_29/11/2021 12:41:46 AM","2021-11-03T23:59:35","Defect","Ship Staff","Ship Staff Insp.","TG/Atmospheric condenser o'bd line N/R Valve body thinned/holed","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","N/R Valve needs to be renewed.Added in REFMAN For DD Jobs","2022-11-13T23:59:35","DLOT220014","Completed","2021-11-10T23:59:35","No","No","No","Internal"]
[null,null,null,23045,null,"27_29/11/2021 12:37:41 AM","2021-11-12T23:59:35","Defect","Ship Staff","Ship Staff Insp.","E/R Light signal columns 12no.partially operatable.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Total 6sets needs to make the 12 no.light signal columns fully operatable.Vsl has received 03complete sets at Singapore on 21st Feb 2022,Spares dismantled from new received Signal columns and Used to rectify Faults in Partially operatable Signal columns-okay","2022-02-11T23:59:35","DLOT215057","Completed","2022-03-04T23:59:35","No","No","No","Internal"]
[null,null,null,23047,null,"27_29/11/2021 12:45:19 AM","2021-11-17T23:59:35","Defect","Ship Staff","Ship Staff Insp.","ODME Fading printouts","Cargo Mach.","MARPOL Related","Equipment Related","6.13","Low","","","New Ribbon catridge recived and replaced, ODME printer printing normal.","2022-02-16T23:59:35","DLOT210230","Completed","2022-02-20T23:59:35","No","No","No","Internal"]
[null,null,null,23048,null,"27_01/12/2021 10:51:30 AM","2021-11-21T23:59:35","Defect","Ship Staff","Ship Staff Insp.","DG2 Alternator drawing high current","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Office informed and Investigation is in progress.","2022-02-20T23:59:35","","Completed","2022-02-17T23:59:35","No","No","No","Internal"]
[null,null,null,23050,null,"27_02/12/2021 5:36:46 AM","2021-11-24T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Ships Elevator inoperational.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.3","Medium","","","Elevetor travells on all deck except \"E\"Deck. RO Raised for E deck , awaiting spares","2022-02-23T23:59:35","DLOT210234","Completed","2021-12-02T23:59:35","No","No","No","Internal"]
[null,null,null,23215,null,"27_27/12/2021 5:33:36 AM","2021-11-29T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Galley Communitator Not Operational from Takeover time of Present Ch Cook","Accommodation","MLC Related","Equipment Related","","","","","As spares are difficult and expensive to source, complete unit must be supplied to rectify the Defect,Presently made operation But unable to Mince the Garbage to the Size required By Regulation.","2022-03-25T23:59:35","DLOT220099","Completed","2022-03-04T23:59:35","No","No","No","Internal"]
[null,null,null,23216,null,"27_27/12/2021 5:40:48 AM","2021-11-29T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Brigde De-Fogger Not Operational","Navigation - Others","Navigation","Equipment Related","","","","","De-Fogger Heating elements renewed,presently working good.","2022-03-25T23:59:35","","Completed","2022-01-13T23:59:35","No","No","No","Internal"]
[null,null,null,23218,null,"27_28/12/2021 3:08:49 AM","2021-11-30T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Bunker/FW Tanks LL Indications in CCR ,Tank Radar Not Showing ","Hull & Tanks","MARPOL Related","Equipment Related","8.15","High","","","Issue resolved with the help of Elect Supt Mr Kamlesh","2022-04-25T23:59:35","","Completed","2022-02-21T23:59:35","No","No","No","Internal"]
[null,null,null,23219,null,"27_28/12/2021 3:13:25 AM","2021-11-30T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Ballast Tanks level Indication for No. of tanks not Working - ( 1W, 2W, 3W etc.)","Hull & Tanks","Cargo / Ballast Systems","Equipment Related","8.15","High","","","Troubleshooting in Progress, Vessel in Ballast condition, to be done in Loaded passage,Minor signal air leaks on LL Indications control lines rectified/Under Observation,","2022-03-25T23:59:35","","Completed","2022-03-07T23:59:35","No","No","No","Internal",""]
[null,null,null,23174,null,"27_12/12/2021 7:47:26 AM","2021-12-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Bunker line isolation valve found leaking , gland packing studs found wasted.","Deck - Pipe / Fittings","Eng. / Strg. Comp.","Equipment Related","11.4","Very High","","","Gland Packing ,Studs and Nuts Renewed-okay","2021-12-13T23:59:35","","Completed","2021-12-05T23:59:35","No","No","No","Internal"]
[null,null,null,23221,null,"27_29/12/2021 5:26:59 AM","2021-12-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Various Pressure gauges not working ( Eductor Drive, Stripping pump, COP # 1 suction etc.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.26","High","","","All pumproom pressure gauges calibrated, all in order","2022-03-01T23:59:35","","Completed","2022-01-22T23:59:35","No","No","No","Internal","Is the problem with gauges or the line. Please remove the gauges and calibrate. raise RO as required."]
[null,null,null,23222,null,"27_29/12/2021 5:30:28 AM","2021-12-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Vapor Line without O2 Sensor","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.42","Medium","","","O2 sensor to install in Drydock, will include in REFMAN as per office instructions","2022-03-01T23:59:35","","Completed","2021-12-25T23:59:35","No","No","No","Internal"]
[null,null,null,23223,null,"27_28/12/2021 3:26:25 AM","2021-12-01T23:59:35","Observation","Ship Staff","Ship Staff Insp.","AE No.3 F.O injection Pumps are due for O'haul.","E/R - Aux. Engine","Eng. / Strg. Comp.","External Factors","","","","","Requisition Raised for required Spares,FO Injection pp's o'hauled with New Received Spares,","2022-03-25T23:59:35","DLOT220009","Completed","2022-03-10T23:59:35","No","No","No","Internal","Spares supplied . Please carryout overhauling"]
[null,null,null,23224,null,"27_29/12/2021 5:36:20 AM","2021-12-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Individual IG pressure readouts for tanks on Bridge are not available","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.19","High","","","Design, Will include in REFMAN as per office instructions","2022-03-01T23:59:35","","Completed","2021-12-25T23:59:35","No","No","No","Internal"]
[null,null,null,23225,null,"27_29/12/2021 5:38:46 AM","2021-12-01T23:59:35","Observation","Ship Staff","Ship Staff Insp.","3S COT  tank valve suspected leaking","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.18","High","","","job entered into REFMAN for DD.","2022-03-01T23:59:35","","Completed","2022-02-26T23:59:35","No","No","No","Internal"]
[null,null,null,23226,null,"27_29/12/2021 5:44:16 AM","2021-12-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","IG main line giving false Low pressure alarm  on IG panel","Inert Gas","Cargo / Ballast Systems","Equipment Related","8.2","Medium","","","rectified","2022-02-01T23:59:35","","Completed","2021-12-08T23:59:35","No","No","No","Internal"]
[null,null,null,23227,null,"27_29/12/2021 5:48:45 AM","2021-12-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Steering gear auto exchange telephone buttons broken","Miscellaneous","Emgcy. Systems","Equipment Related,Human Error","10.16","Very High","","","Replaced","2022-03-01T23:59:35","","Completed","2021-12-13T23:59:35","No","No","No","Internal"]
[null,null,null,23228,null,"27_29/12/2021 5:51:54 AM","2021-12-01T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Hose handling crane pressure gauge not working","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.63","High","","","New pressure gauges installed","2022-03-01T23:59:35","","Completed","2022-01-09T23:59:35","No","No","No","Internal"]
[null,null,null,23230,null,"27_29/12/2021 11:48:21 PM","2021-12-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","2 Light cover in pumproom found cracked","Cargo Mach.","Cargo / Ballast Systems","Equipment Related,Human Error","11.11","Very High","","","renewed","2022-03-01T23:59:35","","Completed","2021-12-07T23:59:35","No","No","No","Internal"]
[null,null,null,23231,null,"27_29/12/2021 11:50:09 PM","2021-12-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Port Side FWD Vapor manifold seat ring is broken.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.42","Medium","","","Port Side FWD Vapor manifold seat ring renewed.","2022-03-01T23:59:35","","Completed","2022-03-05T23:59:35","No","No","No","Internal","Please raise RO at the earliest."]
[null,null,null,23232,null,"27_29/12/2021 11:53:04 PM","2021-12-01T23:59:35","Observation","Ship Staff","Ship Staff Insp.","No stand alone PC + Printer for Surveyor use (Cyber Security)","Miscellaneous","Communication","External Factors,Human Error","7.16","High","","","Will raise RO for Spare PC","2022-03-01T23:59:35","","Completed","2021-12-25T23:59:35","No","No","No","Internal"]
[null,null,null,23233,null,"27_30/12/2021 12:00:57 AM","2021-12-01T23:59:35","Defect","Ship Staff","Ship Staff Insp."," ECDIS (MARIS) - alarmable OE (Object Editor) objects gets deleted from the ENC whenever the ECDIS re-starts due to which we have to plot the OE again & set alarm on it.","Navigation - ECDIS","Navigation","Equipment Related","3.7","Very High","","","Discussed with shore Service engineer, Alarmable OE is not getting saved in OE folder after alarm is set. This is a design issue of manufacturer. ","2022-03-01T23:59:35","","Completed","2022-02-16T23:59:35","No","No","No","Internal"]
[null,null,null,23234,null,"27_30/12/2021 12:05:34 AM","2021-12-01T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Deck Lights getting fused frequently.","Miscellaneous","General Appearance","Equipment Related","11.9","Low","","","Holders and lamps renewed frequently,as per Elect Supt all deck lights to be converted to LED:Added to REFMAN in DD Jobs,","2022-03-01T23:59:35","PO to be raised by Office,","Completed","2021-12-10T23:59:35","No","No","No","Internal"]
[null,null,null,23236,null,"27_30/12/2021 12:12:35 AM","2021-12-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Length of Starboard lifeboat remote lowering wire is short","LSA / FFA","Safety / LSA / FFA","Equipment Related,Human Error","5.27","Medium","","","RO received ( DLOT210220 ). Replaced","2022-03-01T23:59:35","DLOT210220","Completed","2022-02-20T23:59:35","No","No","No","Internal"]
[null,null,null,23237,null,"27_29/12/2021 11:57:16 PM","2021-12-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","2 sets of Bridge STBD wipers not working","Navigation - Others","Navigation","Equipment Related,Human Error","12.1","High","","","Repaired, RO to raise for spares after 1st jAN 2022","2022-02-01T23:59:35","","Completed","2021-12-25T23:59:35","No","No","No","Internal"]
[null,null,null,23723,null,"27_13/01/2022 5:19:09 AM","2022-01-03T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Deck air Compressor Tripping on High Element Temperature...","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related","","","","","Deck Air Compressor Stopped and Cause of Trouble Investigated,Compr Oil seperator /Suction/oil Filter Renewed,Suction vv and Unloader assembly Overhauled,Element Oil Control vv Renewed,LO Sump cleaned and Charged with Fresh oil.Tried out Presently working Good.","2022-01-10T23:59:35","DLOT220047","Completed","2022-01-08T23:59:35","No","No","No","Internal"]
[null,null,null,23823,null,"27_31/01/2022 4:42:42 PM","2022-01-05T23:59:35","Defect","Ship Staff","Ship Staff Insp.","FWG Ejector p/p discharge valve body thinned / holed","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Valve repaired by Build up/Welding in Engine rm w.shop","2022-03-07T23:59:35","DLOT220088","Completed","2022-02-11T23:59:35","No","No","No","Internal","awaiting for quotes."]
[null,null,null,23722,null,"27_15/01/2022 21:14:55","2022-01-09T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Mast Riser Valve leaking","Cargo Mach.","Cargo / Ballast Systems","External Factors","8.19","High","","","Seat ring renewed.","2022-02-01T23:59:35","","Completed","2022-01-14T23:59:35","No","No","No","Internal","Please inspect and raise RO for required spares."]
[null,null,null,23824,null,"27_31/01/2022 4:32:39 PM","2022-01-10T23:59:35","Defect","Ship Staff","Ship Staff Insp.","LT Cooling P/P #1 motor Faulty.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","11.9","Low","","","Motor Checked,Found Damage to stator/Rotor due to Damaged Bearing/Cover","2022-03-10T23:59:35","DLOT220041","Completed","2022-02-23T23:59:35","No","No","No","Internal"]
[null,null,null,24680,null,"27_03/03/2022 7:05:30 PM","2022-02-24T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Ship's Elevator Not Operational due to lack of Required Spare Parts//Invertor","Elect. Mach. & Equip.","MLC Related","Equipment Related","","","","","GOC/GORCards/ PCB's requires Renewal as per Shipstaff TS & Elevator technician's Report, during his Last Visit at Singapore Anchorage on 21st Feb 2022,As per Mater Elevator Tech Additionally Spare Invertor is Required to Rectify the Elevator Defect.\nTECHNICIANS EXPECTED TO BOARD VESSEL ON 18/11/22 AND SAIL FOR WORK ON UPGRADE OF ELEVATOR.\nControl system renewed by technicians. Elevator operational now","2022-11-26T23:59:35","DLOT220020 Raised again on 02nd Jan 2022 Additionally DLOT220125 Also Required Same has been informe","Completed","2022-11-19T23:59:35","No","No","No","Internal","This elevator needs complete upgradation and the office is liaising with Makers to get this done. Current model spares are not in production anymore."]
[null,null,null,24682,null,"27_28/03/2022 5:18:20 PM","2022-03-18T23:59:35","Defect","Ship Staff","Ship Staff Insp.","No.2 deck seal pump suction pipe corroded and has pin hole","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Complete suction pipe renewed","2022-03-26T23:59:35","","Completed","2022-03-19T23:59:35","No","No","No","Internal"]
[null,null,null,24683,null,"27_26/3/2022 7:42:06 AM","2022-03-21T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Unable to put M/E pumps on st-by mode as SAU panel  I/P Board is not operational","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","M/E st-by pumps selected to manual mode due to shortage of spare I/P Card. New I/P Card is required for AMS - SAU panel.","2022-04-25T23:59:35","","Completed","2022-03-22T23:59:35","No","No","No","Internal"]
[null,null,null,23235,null,"27_30/12/2021 12:09:12 AM","2022-03-29T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Bridge rudder angle indicator not matching with the actual rudder angle,this is observed not all times.Error of almost 6° experienced.","Navigation - Others","Navigation","Equipment Related","10.39","High","","","Fault Finding Carried out//Fault has been traced to Rudder Angle Indicator Transmitter Unit & Amplifier Unit,Office Informed and RO Raised for Required Spares//Spares Received and Renewed//Defect rectified","2022-06-27T23:59:35","DLOT220121//220125","Completed","2022-05-01T23:59:35","No","No","No","Internal"]
[null,null,null,23049,null,"27_30/11/2021 7:36:55 AM","2022-04-10T23:59:35","Defect","Ship Staff","Ship Staff Insp.","CCR anemometer display  is not working.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.11","Medium","","","Display to be renewed once Received,New spare received//Formatting carried out by Shore Tech//Mariapps:Okay","2022-07-09T23:59:35","DLOT220063","Completed","2022-05-18T23:59:35","No","No","No","Internal"]
[null,null,null,19554,null,"27_26/05/2021 19:31:02","2022-04-10T23:59:35","Observation","Ship Staff","Nav Audit / Verification","PA system for forward and aft station non-operational","Navigation - Others","Communication","Equipment Related","4.7","High","","","Pending re-investigation.","2023-08-30T23:59:35","","Completed","2023-08-15T23:59:35","No","No","No","Internal","What was found in the troubleshooting? Please write full detail here and send mail. Will supply Spares accordingly based on the trouble shooting."]
[null,null,null,23220,null,"27_28/12/2021 3:21:46 AM","2022-04-10T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Prov.Ref Compressor No.2 Not Able to maintain Required Refer rm Temps,","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","02pcs Spare Used Prov Ref Comp. complete landed at Singapore to HMS For Re-conditioning on 21st FEB 2022:Re-cond comp received//Renewed:Okay","2022-07-09T23:59:35","DLOT220018","Completed","2022-04-25T23:59:35","No","No","No","Internal"]
[null,null,null,23229,null,"27_29/12/2021 11:45:10 PM","2022-04-10T23:59:35","Defect","Ship Staff","Ship Staff Insp.","No.1 Foam monitor valves found leaking","LSA / FFA","Safety / LSA / FFA","Equipment Related,Human Error","5.35","Medium","","","No.1 Foam Monitor Valve Renewed","2022-07-09T23:59:35","DLOT220092","Completed","2022-06-11T23:59:35","No","No","No","Internal"]
[null,null,null,18678,null,"27_17/04/2021 4:21:13 PM","2022-04-10T23:59:35","Critical Equipment","Ship Staff","Ship Staff Insp.","DG3 FCU Breaker  no1&2 not connected to ES1 for remote trip operation","Critical Equip.","Safety / LSA / FFA","Equipment Related","5.35","Medium","","","New MCB has been renewed for DG-3 FCU unit and trip circuit connected to ES1","2022-07-09T23:59:35","DLOT210084//220130","Completed","2022-05-04T23:59:35","No","No","No","Internal"]
[null,null,null,26250,null,"27_28/06/2022 3:50:32 PM","2022-06-05T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Refer system has gas leak","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Entire system needs to check for gas leak including pressure testing of condensor.Gas leak has been rectified. Refrigration plant working satisfactorily.","2022-07-26T23:59:35","","Completed","2022-07-26T23:59:35","No","No","No","Internal"]
[null,null,null,26251,null,"27_28/06/2022 3:54:15 PM","2022-06-05T23:59:35","Defect","Ship Staff","Ship Staff Insp.","E/R blower No.4 impeller damaged ","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","New impeller to install once receive spare. Spare received at Singapore, Fan impeller renewed with spare. Fan tried out, satisfactory.","2022-07-25T23:59:35","DLOT 220163","Completed","2022-07-19T23:59:35","No","No","No","Internal"]
[null,null,null,26252,null,"27_28/06/2022 3:57:46 PM","2022-06-10T23:59:35","Defect","Ship Staff","Ship Staff Insp.","No.1 L.T cooler backwash valve body corroded and holed","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","L.T cooler valve needs to replace with spare valve. LT cooler backflushing valve is replaced with spare valve. ","2022-07-25T23:59:35","DLOT 220180 raised","Completed","2022-07-25T23:59:35","No","No","No","Internal"]
[null,null,null,26253,null,"27_28/06/2022 4:00:01 PM","2022-06-10T23:59:35","Defect","Ship Staff","Ship Staff Insp.","C.O.P warm up valves leaking","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Valves needs to replace with spare valves. Spares received, shall complete this on priority,","2022-09-11T23:59:35","DLOT 220180","Completed","2022-09-10T23:59:35","No","No","No","Internal","Spares have been supplied and valves need to be changed at the earliest."]
[null,null,null,26254,null,"27_28/06/2022 4:58:19 PM","2022-06-12T23:59:35","Defect","Ship Staff","Ship Staff Insp.","No.3 Foam Monitor Valve Leaking","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.35","Medium","","","4 New Gate Valves received at Singapore on 23 July 2022.NO.3 Foam Monitor Valve Renewed & tried out on 02 Aug 2022","2022-07-26T23:59:35","DLOT220092 : GATE VALVES FOR FOAM MONITORS @ SINGAPORE","Completed","2022-07-28T23:59:35","No","No","No","Internal"]
[null,null,null,26255,null,"27_28/06/2022 5:03:05 PM","2022-06-12T23:59:35","Critical Equipment","Ship Staff","Ship Staff Insp.","LED Failure Alarm on ODME.Suspected Detector Unit Faulty","Critical Equip.","MARPOL Related","Equipment Related","6.13","Low","","","ODME DETECTOR UNIT RENEWED","2022-07-26T23:59:35","DLOT220117 : ODME DETECTOR UNIT","Completed","2022-07-22T23:59:35","No","No","No","Internal"]
[null,null,null,26249,null,"27_28/06/2022 5:27:49 PM","2022-06-13T23:59:35","Critical Equipment","Ship Staff","Ship Staff Insp.","Few Lifeboat Seatbelts found damaged","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.29","High","","","23 Lifeboat seat belts renewed","2022-07-26T23:59:35","DLOT220171-Lifeboat Safety Seatbelts","Completed","2022-07-22T23:59:35","No","No","No","Internal"]
[null,null,null,26256,null,"27_28/06/2022 5:24:44 PM","2022-06-13T23:59:35","Other","Ship Staff","Ship Staff Insp.","Draft Gauge showing Erratic Readings","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.2","Medium","","","Draft Gauge Attended by Emerson Technician at Singapore.\nDraft Gauge working satisfactory.","2022-09-25T23:59:35","DLOT220192 - CCR DRAFT GAUGE MODULE","Completed","2022-09-20T23:59:35","No","No","No","Internal","Troubleshooting in progress with makers. If required we will send SE in Singapore."]
[null,null,null,26257,null,"27_30/06/2022 05:30:45","2022-06-14T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Stbd Lifeboat Compass showing incorrect reading","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.29","High","","","Port & Stbd Lifeboat Compass renewed","2022-07-26T23:59:35","DLOT 220178 - Lifeboat Magnetic Compass","Completed","2022-07-23T23:59:35","No","No","No","Internal"]
[null,null,null,26258,null,"27_30/06/2022 05:35:01","2022-06-14T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Fwd Embrakation ladder found damaged & deteriorated","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.47","Medium","","","Fwd Embarkation ladder renewed","2022-08-25T23:59:35","DLOT220188 - Embarkation & Pilot ladder@ Singapore","Completed","2022-07-21T23:59:35","No","No","No","Internal"]
[null,null,null,26265,null,"27_30/06/2022 05:37:53","2022-06-14T23:59:35","Observation","Ship Staff","Ship Staff Insp.","3S COT Valve found Leaking","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.18","High","","","3S COT Main Valve CAV 126 & CAV 175 Seat Ring found damaged & Renewed.3S COT Stripper Valve CAV 143 & CAV 198 inspected,seat ring found intact.","2022-07-26T23:59:35","","Completed","2022-07-11T23:59:35","No","No","No","Internal"]
[null,null,null,26259,null,"27_30/06/2022 05:41:22","2022-06-15T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Mooring Winch  & Windlass gear oil found emulsified & sight glass found opaque","Deck - Machinery","Mooring","Equipment Related","9.14","Medium","","","Gear Oil for Windlass W1 & W2 renewed & sight glass cleaned. Cleaning of Mooring Winch Sight Glasses completed. MW M1 Gear oil renewed.","2022-08-26T23:59:35","","Completed","2022-08-25T23:59:35","No","No","No","Internal","Noted."]
[null,null,null,26260,null,"27_30/06/2022 05:45:00","2022-06-15T23:59:35","Observation","Ship Staff","Ship Staff Insp.","M2 mooring winch block leaking","Deck - Machinery","Mooring","Equipment Related","9.14","Medium","","","Temporary Repairs done.Holding for past 3 months. New spare received kept standby\n","2022-09-26T23:59:35","DLOT220148 : Mooring Winch(M2),two speed valve","Completed","2022-09-21T23:59:35","No","No","No","Internal"]
[null,null,null,26261,null,"27_30/06/2022 05:47:11","2022-06-16T23:59:35","Observation","Ship Staff","Ship Staff Insp.","RX-8700 Gas meter sensor Renewal Overdue","Miscellaneous","Cargo / Ballast Systems","Human Error","5.23","Very High","","","O2 / H2S Low/H2s High - Sensors renewed","2022-07-26T23:59:35","","Completed","2022-07-23T23:59:35","No","No","No","Internal"]
[null,null,null,26266,null,"27_17/07/2022 18:38:20","2022-07-04T23:59:35","Observation","Ship Staff","Ship Staff Insp.","2C COT Valves suspected leaking","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.18","High","","","2C COT Main Valve CAV 114 inspected.Seat Ring found intact.2C Stripper Valve CAV 141 seat ring found damaged & renewed","2022-07-26T23:59:35","","Completed","2022-07-08T23:59:35","No","No","No","Internal"]
[null,null,null,26262,null,"27_17/07/2022 18:50:40","2022-07-07T23:59:35","Observation","Ship Staff","Ship Staff Insp.","IG BRANCH VALVES-1W,SLOP P,SLOP S ,1C & 3C LEAKING","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.2","Medium","","","1P/1S/1C/3C IG Valve Seat Ring Renewed            .Slop S Seat Ring found intact,Valve Disc found damaged.Slop S Complete IG Valve renewed  ","2022-08-26T23:59:35","","Completed","2022-07-28T23:59:35","No","No","No","Internal"]
[null,null,null,26263,null,"27_18/7/2022 9:57:35 AM","2022-07-11T23:59:35","Defect","Ship Staff","Ship Staff Insp.","M/E RPLS Power supply unit defective. The st-by power supply is inuse","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Requisition raised, awaiting spare. Spare received. Shall renew  once vessel is at port. Renewed when vessel was at discharge port","2022-09-26T23:59:35","DLOT220202","Completed","2022-09-12T23:59:35","No","No","No","Internal","VIQ not updated \nSpare has already been supplied in Singapore in July."]
[null,null,null,26264,null,"27_18/07/2022 4:54:10 PM","2022-07-11T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Void Space Vent head covers wasted","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","Equipment Related","2.9","Medium","","","Void Space Vent head covers fabricated","2022-08-10T23:59:35","","Completed","2022-08-09T23:59:35","No","No","No","Internal"]
[null,null,null,26550,null,"27_02/08/2022 5:09:19 PM","2022-07-17T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Renewal of Mats in ER near the electrical panels","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Human Error","6.4","High","","","Need to raise RO for new insulation mats. RO raised DLOT220225\nMats renewed.","2022-09-26T23:59:35","DLOT220225","Completed","2022-09-22T23:59:35","No","No","No","Internal","Raise RO asap so that it can be supplied in Singapore."]
[null,null,null,26551,null,"27_02/08/2022 4:34:35 PM","2022-07-17T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Several MSDS for chemicals and gases were found to be several years old. Please take a printout of the latest MSDS and replace it.","Documentation","Eng. / Strg. Comp.","Human Error","5.46","Medium","","","MSDS printout to be taken. Print out of latest version of MSDS taken and filed.","2022-08-17T23:59:35","","Completed","2022-08-11T23:59:35","No","No","No","Internal","All new MSDS have been downloaded and put in the infinity folder for vessels to print out and replace. Ensure all are updated onboard."]
[null,null,null,26552,null,"27_02/08/2022 4:51:23 PM","2022-07-17T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ME JCW pump no.2 found leaking from mechanical seal","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","ME jacket cooling HT pump No 2 overhauled and the seal was renewed.","2023-06-27T23:59:35","DLOT220198","Completed","2023-03-09T23:59:35","No","No","No","Internal","Item already in SG warehouse and will be supplied during your Singapore call."]
[null,null,null,26553,null,"27_02/08/2022 4:59:49 PM","2022-07-17T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","COPT Main steam stop valve found leaking. Noticed a bucket kept underneath the valve.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Leak to be identified and if required RO to be raised. Leak was from the gland. Gland packing renewed and leak is arrested.","2022-08-16T23:59:35","","Completed","2022-08-10T23:59:35","No","No","No","Internal","This should have been identified by now. Is it from the bonnet? Does the vessel have a bonnet gasket onboard."]
[null,null,null,26557,null,"27_02/08/2022 3:48:46 PM","2022-07-17T23:59:35","Non Conformity","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Noticed that various permits submitted to CE for signature were without completely filled by the officer incharge","Documentation","Cert. & Docu.","Human Error","5.2","Very High","","","All permits checked and each entry filled properly before submitting to CE for his signature","2022-07-19T23:59:35","","Completed","2022-07-19T23:59:35","No","No","No","Internal"]
[null,null,null,26558,null,"27_02/08/2022 3:53:01 PM","2022-07-17T23:59:35","Non Conformity","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ER movement book not updated after Arr/Dep port. Signature of CE found missing","Documentation","Cert. & Docu.","Human Error","4.2","Medium","","","Movement book checked and CE signature taken in all pages.","2022-07-19T23:59:35","","Completed","2022-07-19T23:59:35","No","No","No","Internal"]
[null,null,null,26559,null,"27_02/08/2022 4:05:31 PM","2022-07-17T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Hand wheel found missing on the v/v for stm injection for Hot well.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Human Error","11.5","Medium","","","Hand wheel renewed.","2022-08-01T23:59:35","","Completed","2022-08-21T23:59:35","No","No","No","Internal"]
[null,null,null,26560,null,"27_02/08/2022 4:09:01 PM","2022-07-17T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Oil leak was observed from AE no.2. Leaks to be identified and rectified.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Leak found from LO glacier/centrifugal filter connection. Same rectified by renewing the Cu washer and by tightening the connection.","2022-07-24T23:59:35","","Completed","2022-07-22T23:59:35","No","No","No","Internal"]
[null,null,null,26561,null,"27_02/08/2022 4:01:32 PM","2022-07-17T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Cable stack in ECR computer table is in a mess. Needs to arrange and laid out properly.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Human Error","10.37","Medium","","","All cables laid properly and tied with cable tie neatly.","2022-08-01T23:59:35","","Completed","2022-07-20T23:59:35","No","No","No","Internal"]
[null,null,null,26562,null,"27_02/08/2022 3:57:48 PM","2022-07-17T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ECR AC No.1&2 evaporator fins found in dirty condition. Even felt filter was dirty. Same to be cleaned.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","ECR both AC evaporator fins water washed/cleaned and felt filter renewed with spare.","2022-07-24T23:59:35","","Completed","2022-07-21T23:59:35","No","No","No","Internal"]
[null,null,null,26563,null,"27_02/08/2022 4:11:52 PM","2022-07-17T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Thermometer mounted on AE no.2 exhaust line found to have turned completely black","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Thermometer renewed with spare.","2022-08-01T23:59:35","","Completed","2022-07-23T23:59:35","No","No","No","Internal"]
[null,null,null,26564,null,"27_02/08/2022 4:16:45 PM","2022-07-17T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Several p/p's in ECR found running in MANUAL mode. All pumps to be operated in AUTO mode and standby pumps should be in stby mode","E/R - Pumps","Eng. / Strg. Comp.","Human Error","10.32","Very High","","","All pumps in ECR changed to AUTO mode and all standby pumps put in stby mode.","2022-07-20T23:59:35","","Completed","2022-07-19T23:59:35","No","No","No","Internal"]
[null,null,null,26565,null,"27_02/08/2022 4:20:25 PM","2022-07-17T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Space heaters for several electric motors found to be in OFF position. Engineer are not aware of this.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","All space heaters checked and switched ON.","2022-07-24T23:59:35","","Completed","2022-07-21T23:59:35","No","No","No","Internal"]
[null,null,null,26566,null,"27_02/08/2022 4:38:25 PM","2022-07-17T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Fixed grinding machine-Grinding wheel gap is beyond permissible limit and is very unsafe. Needs to adjust for both buffing and grinding wheel.","Miscellaneous","Eng. / Strg. Comp.","Human Error","","","","","Gap adjusted for both grinding and buffing wheel.","2022-07-24T23:59:35","","Completed","2022-07-22T23:59:35","No","No","No","Internal"]
[null,null,null,26567,null,"27_02/08/2022 4:42:06 PM","2022-07-17T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","External flexible air duct found installed for the service air compressor. Any reason for this?","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Flexible air duct is removed. It was installed when one of the ER fan was not working and ER temperature was higher than normal.","2022-08-01T23:59:35","","Completed","2022-07-24T23:59:35","No","No","No","Internal"]
[null,null,null,26568,null,"27_02/08/2022 4:45:43 PM","2022-07-17T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","No liquid was found in ME T/C and air cooler manometer.","E/R - Main Engine","Eng. / Strg. Comp.","Human Error","10.32","Very High","","","ME turbocharger and air cooler manometer filled with liquid.","2022-07-24T23:59:35","","Completed","2022-07-23T23:59:35","No","No","No","Internal"]
[null,null,null,26569,null,"27_02/08/2022 5:03:03 PM","2022-07-17T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Grease pots of all three COPT's need to be topped up due to low grease quantity in them","Cargo Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Grease pots of all three COPT's topped up.","2022-07-24T23:59:35","","Completed","2022-07-23T23:59:35","No","No","No","Internal"]
[null,null,null,26570,null,"27_02/08/2022 4:27:16 PM","2022-07-17T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Scupper pipe coming from one platform above ECR and between ECR bulkhead and hot well found in bad condition. Needs to be renewed.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Scupper pipe to be fabricated and renewed. New scupper pipe fabricated and fitted in place.","2022-08-17T23:59:35","","Completed","2022-07-29T23:59:35","No","No","No","Internal"]
[null,null,null,26571,null,"27_02/08/2022 5:06:31 PM","2022-07-17T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Several sounding pipes counterweight arrangement are not as per the original. They seem to have been modified and not in good condition.","Miscellaneous","Eng. / Strg. Comp.","Human Error","10.26","High","","","Need to check with the drawing. Sounding pipes with defective counter weights has been rectified.","2022-08-01T23:59:35","","Completed","2022-08-03T23:59:35","No","No","No","Internal"]
[null,null,null,26548,null,"27_30/07/2022 12:36:42 PM","2022-07-18T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Spot rust found near Midship Area Main deck below Crossover valves","Deck - Pipe / Fittings","General Appearance","External Factors","11.3","Medium","","","Spot Derusting & Painting near Midship Area Main deck below Crossover valves completed","2022-09-06T23:59:35","","Completed","2022-09-05T23:59:35","No","No","No","Internal"]
[null,null,null,26549,null,"27_30/07/2022 12:47:27 PM","2022-07-18T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","All Mooring Tails & ropes in use to be marked","Deck - Mooring Machinery","Mooring","Behaviour Based","9.17","High","","","Marking of Mooring Tails & Ropes completed","2022-08-26T23:59:35","","Completed","2022-08-25T23:59:35","No","No","No","Internal","Noted. Once completed update the same."]
[null,null,null,26554,null,"27_02/08/2022 9:08:50 PM","2022-07-18T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Emergency Generator Steps to be added in REFMAN for DD jobs","Miscellaneous","Structural Condn. / WT integrity ","Equipment Related","","","","","Emergency Generator Steps job added in REFMAN","2022-08-26T23:59:35","","Completed","2022-08-15T23:59:35","No","No","No","Internal","ADD it in REFMAN and close it out from DDRL by marking it to DRYDOCK"]
[null,null,null,26556,null,"27_02/08/2022 12:45:30 PM","2022-07-18T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Few Mechanical & Natural Vents around accomodation found dirty","Accommodation","Structural Condn. / WT integrity ","Equipment Related","","","","","Vents cleaned","2022-09-10T23:59:35","","Completed","2022-08-28T23:59:35","No","No","No","Internal","VIQ number not added. \nJob to be taken up on priority and completed."]
[null,null,null,26572,null,"27_30/07/2022 11:35:53 AM","2022-07-18T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Port & Stbd Midship Crane Pressure gauge glass found opaque.","Deck - Machinery","Cargo / Ballast Systems","Equipment Related","","","","","Port & Stbd Midship Crane Pressure Gauge renewed","2022-07-26T23:59:35","","Completed","2022-07-22T23:59:35","No","No","No","Internal"]
[null,null,null,26573,null,"27_30/07/2022 12:45:35 PM","2022-07-18T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Windlass & Winch Brake Markings to be adjusted","Deck - Mooring Machinery","Mooring","Equipment Related","","","","","P & S Windlass & all Mooring Winch Brake Markings checkd & adjusted as required","2022-07-26T23:59:35","","Completed","2022-07-24T23:59:35","No","No","No","Internal"]
[null,null,null,26574,null,"27_30/07/2022 12:49:15 PM","2022-07-18T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Chain Locker Stencil Marking missing","Miscellaneous","General Appearance","Behaviour Based","","","","","Chain Locker P & S Marking completed","2022-07-26T23:59:35","","Completed","2022-07-23T23:59:35","No","No","No","Internal"]
[null,null,null,26575,null,"27_30/07/2022 1:12:20 PM","2022-07-18T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","IMO Symbol for lifebuoy missing near 2S WBT","LSA / FFA","Safety / LSA / FFA","Human Error","","","","","IMO Symbol posted.All IMO symbols checked ","2022-07-26T23:59:35","","Completed","2022-07-20T23:59:35","No","No","No","Internal"]
[null,null,null,26576,null,"27_30/07/2022 1:15:44 PM","2022-07-18T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Neoprene buckets missing in SOPEP Locker","Miscellaneous","MARPOL Related","Behaviour Based,Human Error","","","","","Neoprene Buckets marked & kept in SOPEP locker as per inventory.Crew Members briefed","2022-07-26T23:59:35","","Completed","2022-07-20T23:59:35","No","No","No","Internal"]
[null,null,null,26577,null,"27_30/07/2022 1:18:01 PM","2022-07-18T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Lifeboat Remote Wire to be greased","LSA / FFA","Safety / LSA / FFA","Behaviour Based","","","","","Port & Stbd Lifeboat Remote Wire Greased.Sheaves cleaned.","2022-07-26T23:59:35","","Completed","2022-07-24T23:59:35","No","No","No","Internal"]
[null,null,null,26578,null,"27_30/07/2022 11:32:35 AM","2022-07-18T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Port Gangway Sheave found seized","Deck - Machinery","Safety / LSA / FFA","Equipment Related","","","","","Sheave removed,cleaned & greased.Grease nipple renewed.Checked for movement after boxing up","2022-07-26T23:59:35","","Completed","2022-07-21T23:59:35","No","No","No","Internal"]
[null,null,null,26579,null,"27_30/07/2022 1:20:10 PM","2022-07-18T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Lifeboat Limit Switch Rollers to be freed","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","Port & Stbd Limit Switches checked.Rollers checked for free movement.Repairs done as required","2022-07-26T23:59:35","","Completed","2022-07-24T23:59:35","No","No","No","Internal"]
[null,null,null,26580,null,"27_30/07/2022 1:24:40 PM","2022-07-18T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Few Valve Stencil missing in pumproom","Miscellaneous","General Appearance","Behaviour Based","","","","","Valve stenciling done.All Valves in pumproom checked for prpoer marking & stencil","2022-07-26T23:59:35","","Completed","2022-07-24T23:59:35","No","No","No","Internal"]
[null,null,null,26581,null,"27_02/08/2022 12:43:31 PM","2022-07-18T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","FW Valve at Port Upper Deck Entrance found leaking","Deck - Pipe / Fittings","General Appearance","Equipment Related","","","","","FW Valve Renewed","2022-07-26T23:59:35","","Completed","2022-07-26T23:59:35","No","No","No","Internal"]
[null,null,null,26582,null,"27_30/07/2022 12:55:17 PM","2022-07-18T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Check Mooring Winch M1 return line for Soft patch","Deck - Mooring Machinery","Mooring","Equipment Related","","","","","Mooring winch M1 return line derusted,no soft patch found","2022-07-26T23:59:35","","Completed","2022-07-25T23:59:35","No","No","No","Internal"]
[null,null,null,26583,null,"27_02/08/2022 12:47:09 PM","2022-07-18T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Food garbage drums on the poop deck were found to be lashed with soft rope","Miscellaneous","General Appearance","Behaviour Based","","","","","Food Garbage drums wire lashed","2022-07-26T23:59:35","","Completed","2022-07-26T23:59:35","No","No","No","Internal"]
[null,null,null,26584,null,"27_02/08/2022 12:50:16 PM","2022-07-18T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","An oil drum in the VRCS room was found kept on the bare floor. No MSDS could be located for the Lub oil. ","Miscellaneous","General Appearance","Behaviour Based","","","","","Oil drum kept on wooden pallet & wire lashed.Latest MSDS posted","2022-08-02T23:59:35","","Completed","2022-07-31T23:59:35","No","No","No","Internal"]
[null,null,null,26585,null,"27_30/07/2022 12:42:08 PM","2022-07-18T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","1P PV Valve leaking from Vacuum Side","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.41","Medium","","","1P PV Valve overhauling carried out","2022-08-26T23:59:35","","Completed","2022-07-30T23:59:35","No","No","No","Internal"]
[null,null,null,26586,null,"27_30/07/2022 12:51:05 PM","2022-07-18T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Fwd Store Winch Hydraulic Motor lifting Eye Ring SWL marking missing","Deck - Mooring Machinery","General Appearance","Behaviour Based","8.5","Very High","","","SWL marking done below Eye Ring","2022-08-26T23:59:35","","Completed","2022-08-04T23:59:35","No","No","No","Internal"]
[null,null,null,26587,null,"27_30/07/2022 1:22:00 PM","2022-07-18T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Stbd Void Space Sensor Cover Wasted","Hull & Tanks","Structural Condn. / WT integrity ","Equipment Related","2.9","Medium","","","New Cover Fabricated & boxed up","2022-08-26T23:59:35","","Completed","2022-08-03T23:59:35","No","No","No","Internal"]
[null,null,null,26588,null,"27_30/07/2022 12:43:51 PM","2022-07-18T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Stbd Windlass Hydraulic Hoses to be checked","Deck - Mooring Machinery","Mooring","Equipment Related","9.2","Very High","","","Hydraulic hoses of Windlass & Winches inspected","2022-08-26T23:59:35","","Completed","2022-08-05T23:59:35","No","No","No","Internal"]
[null,null,null,26590,null,"27_02/08/2022 12:48:17 PM","2022-07-18T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Several garbage drum metallic covers were found to be wasted and corroded","Miscellaneous","General Appearance","Behaviour Based","","","","","5 Garbage Drum Lids renewed","2022-08-10T23:59:35","","Completed","2022-07-27T23:59:35","No","No","No","Internal"]
[null,null,null,26589,null,"27_02/08/2022 6:12:07 PM","2022-07-26T23:59:35","Breakdown,Critical Equipment","Ship Staff","Ship Staff Insp.","Pump room blower no.2 shaft coupling found sheared off on starting the fan.","Critical Equip.","Safety / LSA / FFA","Equipment Related","5.18","High","","","RO has been raised for the broken coupling. Need to replace the coupling once spare received. Found spare shaft coupling onboard, same is replaced. Pump room blower tried out, running satisfactorily.","2022-08-26T23:59:35","RO - DLOT220221","Completed","2022-08-05T23:59:35","No","No","No","Internal"]
[null,null,null,26555,null,"27_02/08/2022 9:19:07 PM","2022-07-28T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Slop P IG Valve Disc found damaged.No spare Onboard","Inert Gas","Cargo / Ballast Systems","Equipment Related","8.2","Medium","","","Slop P IG Valve renewed","2022-09-25T23:59:35","DLOT 220222 - IG BRANCH VALVES","Completed","2022-09-25T23:59:35","No","No","No","Internal","Spares have been shipped from China and will be supplied at next Singapore call."]
[null,null,null,26591,null,"27_03/08/2022 12:15:34 PM","2022-07-28T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Pumproom Fixed Gas Detection System O2 Sensor showing Erratic Reading","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","O2 Sensor Renewed on 02 Aug 2022.Working Satisfactory.","2022-07-28T23:59:35","","Completed","2022-07-28T23:59:35","No","No","No","Internal"]
[null,null,null,26685,44428,"27_Thu Sep 01 2022 20:00:38 GMT+0800","2022-08-25T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Ballast Valve BEV 30 Indicator Barrier unit faulty","Elect. Mach. & Equip.","Cargo / Ballast Systems","Equipment Related","","","","","Barrier unit to be renewed.","2023-04-29T23:59:35","DLOT 220228 - VALVE POSITION INDICATION- ZENER BARRIER\nDLOT 230024- Indicator units","Completed","2023-03-26T23:59:35","No","No","No","Internal"]
[null,null,null,26686,93309,"27_Thu Sep 01 2022 20:02:57 GMT+0800","2022-08-25T23:59:35","Observation","Ship Staff","Ship Staff Insp.","APK BWTS System Flow Control Valve PCB defective","E/R - Pipes/ valves & fittings","Cargo / Ballast Systems","Equipment Related","","","","","Flow Control Valve PCB to be renewed. SPARE AWAITED, DUE DATE POSTPONED. controller renewed after receipt.","2022-12-27T23:59:35","DLOT 220229 - PTM FOR FCV 3131- BWTS (AFT)","Completed","2022-11-18T23:59:35","No","No","No","Internal"]
[null,null,null,26687,13473,"27_Fri Sep 02 2022 10:45:05 GMT+0800","2022-08-25T23:59:35","Observation","Ship Staff","Ship Staff Insp.","ME LO AUTO BACKWASH FILTER HYDRAULIC MOTOR TURNING INDICATOR NOT WORKING","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","HYDRAULIC MOTOR RATCHET HELICAL GROOVE IS WORN OUT. NEED TO REPLACE RATCHET WITH SPARE. \nRatchet renewed.","2022-10-16T23:59:35","","Completed","2022-09-08T23:59:35","No","No","No","Internal"]
[null,null,null,27259,44523,"27_Sun Oct 02 2022 19:27:59 GMT+0800","2022-09-03T23:59:35","Observation","Ship Staff","Ship Staff Insp.","ODME MAIN CONTROL PCB  GETTING TRIP DUE TO OVERHEATING","Critical Equip.","Cargo / Ballast Systems","Equipment Related","","","","","AWAITING SPARE- DUE DATE POSTPONED AWAITING SPARE. PCB received and same renewed. Awaiting test result. Tested during annuals at Khorfakkan.","2022-12-27T23:59:35","DLOT225053 - ODME MAIN CONTROL PCB ","Completed","2022-12-05T23:59:35","No","No","No","Internal"]
[null,null,null,27257,40736,"27_Sun Oct 02 2022 20:38:06 GMT+0800","2022-09-13T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","CCR BWTS Panel Boot Failure","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","Troubleshooting in progress.\nAwaiting Recovery Software from Makers.\nService engineer expected in Khorfakkan to solve the problem\nService engineer intervention provided temporary solution. After operation sam problem resurfaced. Service engineer visited vessel at San Diego with new SSD and cable. System was under observation for stability. Working well. ","2023-03-28T23:59:35","","Completed","2023-02-14T23:59:35","No","No","No","Internal"]
[null,null,null,27258,88742,"27_Sun Oct 02 2022 19:30:03 GMT+0800","2022-09-14T23:59:35","Observation","Ship Staff","Ship Staff Insp.","IG EXTRA LOW FAULTY ALARM","Inert Gas","Cargo / Ballast Systems","Equipment Related","","","","","TROUBLESHOOTING IN PROGRESS. Initial troubleshooting mail sent on 22/09/22. Reply awaited.\nLL trip and LL pressure switch renewed on 12/10/2022. Will be checked in operation during pre- arrival test planned for 24th October.After testing will mark it complete. Checked, working well","2022-10-16T23:59:35","","Completed","2022-10-20T23:59:35","No","No","No","Internal"]
[null,null,null,27260,66285,"27_Sun Oct 02 2022 19:33:22 GMT+0800","2022-09-14T23:59:35","Observation","Ship Staff","Ship Staff Insp.","MOORING WINCH M5 OPERATING LEVER FAULTY. MOORING WINCH KEEPS ROTATING EVEN IN NEUTRAL POSITION AFTER OPERATING FOR FEW MINUTES. THERE IS TIME LAG INCASE WINCH IS OPERATED FURTHER FOR LOWERING OR HEAVING.","Deck - Mooring Machinery","Mooring","Equipment Related","9.14","Medium","","","The block was overhauled in Panama and fitted. Tried out  working satisfactorily.","2023-03-28T23:59:35","DLOT220240 - MOORING WINCH SPARES","Completed","2023-03-14T23:59:35","No","No","No","Internal"]
[null,null,null,27261,87143,"27_Sun Oct 02 2022 19:31:39 GMT+0800","2022-09-14T23:59:35","Observation","Ship Staff","Ship Staff Insp.","MW M6B HYDRAULIC BRAKE CYLINDER LEAKING","Deck - Mooring Machinery","Mooring","Equipment Related","","","","","MW M6B BRAKE CYLINDER  RENEWED","2022-10-02T23:59:35","","Completed","2022-09-30T23:59:35","No","No","No","Internal"]
[null,null,null,27263,20633,"27_Sun Oct 02 2022 19:37:17 GMT+0800","2022-09-20T23:59:35","Observation","Ship Staff","Ship Staff Insp.","MOORING WINCH M6B WIRE TO BE RENEWED","Deck - Mooring Machinery","Mooring","Equipment Related","","","","","WIRE RENEWED & GREASED","2022-09-26T23:59:35","","Completed","2022-09-22T23:59:35","No","No","No","Internal"]
[null,null,null,27264,18859,"27_Sat Oct 15 2022 19:53:16 GMT+0800","2022-09-20T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ME both air cooler housing to de-rust and paint.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","ME air cooler housing to be chipped/de-rusted and painted in Panama","2023-03-27T23:59:35","","Completed","2023-03-14T23:59:35","No","No","No","Internal"]
[null,null,null,27284,40478,"27_Sat Oct 15 2022 19:40:57 GMT+0800","2022-09-20T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ME revolution meter at the local maneuvering station not showing zero rpm when the vessel is at stand still. Revolution needs to be matched with bridge and ECR gauge","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Adjusted the needle to zero when main engine stopped.","2023-04-14T23:59:35","","Completed","2023-04-13T23:59:35","No","No","No","Internal"]
[null,null,null,27287,10628,"27_Sat Oct 15 2022 13:32:56 GMT+0800","2022-09-20T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Mushroom vents OPEN / CLOSE indicators all around accommodation to be painted RED or YELLOW for ease of identification. ","Accommodation","General Appearance","Behaviour Based","","","","","Indicator marking completed.","2022-11-26T23:59:35","","Completed","2022-11-10T23:59:35","No","No","No","Internal"]
[null,null,null,27288,81443,"27_Sat Oct 15 2022 13:35:36 GMT+0800","2022-09-20T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Visual alarm indicator for the new anemometer in the CCR was not installed. Same needs to be installed. ","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","Visual Alarm indicator to be installed. Our model does not seem to have visual indicator as per the manual. Mail sent to office in this regard. Awaiting response to the mail. Inbuilt visual indicator in display. No external indicator required.","2023-03-27T23:59:35","","Completed","2023-01-31T23:59:35","No","No","No","Internal"]
[null,null,null,27289,60382,"27_Sat Oct 15 2022 13:29:27 GMT+0800","2022-09-20T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","PPE in the Battery locker found in dismal state. They need to cleaned and damaged PPE gear is to be replaced with new. ","Miscellaneous","General Appearance","Behaviour Based","","","","","PPE Renewed","2022-10-11T23:59:35","","Completed","2022-10-08T23:59:35","No","No","No","Internal"]
[null,null,null,27292,56020,"27_Sat Oct 15 2022 13:31:12 GMT+0800","2022-09-20T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Latches for the emergency escape hatch from the elevator trunk on the Bridge wing found very hard. In case of emergency, it will be very hard to open from inside in case of an emergency. Same needs to be eased and greased up. ","Elect. Mach. & Equip.","Emgcy. Systems","Equipment Related","","","","","Latches eased up & greased","2022-10-11T23:59:35","","Completed","2022-10-10T23:59:35","No","No","No","Internal"]
[null,null,null,27293,86143,"27_Sat Oct 15 2022 16:25:14 GMT+0800","2022-09-20T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","MSDS for batteries in the battery locker found to be updated and not maker specific. Same needs to be renewed.","Navigation - GMDSS & Communication","Safety / LSA / FFA","Human Error","5.46","Medium","","","Maker specific MSDS to be downloaded and renewed.\nMaintenance free battery MSDS downloaded and placed. Maker specific not available on internet. Mail sent in this regard","2022-10-16T23:59:35","","Completed","2022-10-03T23:59:35","No","No","No","Internal"]
[null,null,null,27294,91497,"27_Sat Oct 15 2022 16:29:36 GMT+0800","2022-09-20T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Dead man alarm activation key at the entrance of Engine Room from changing locker found missing","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Human Error","10.4","High","","","Key to be put in place. Key found and put in place. Mail sent in this regard ","2022-10-20T23:59:35","","Completed","2022-10-12T23:59:35","No","No","No","Internal"]
[null,null,null,27295,91522,"27_Sat Oct 15 2022 13:34:33 GMT+0800","2022-09-20T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Port side aft scupper on the Monkey Island found choked. Water accumulation was noted. ","Accommodation","General Appearance","Equipment Related","","","","","Accomodation scuppers checked & chocked lines cleared","2022-10-20T23:59:35","","Completed","2022-10-08T23:59:35","No","No","No","Internal"]
[null,null,null,27262,57078,"27_Sun Oct 02 2022 19:36:00 GMT+0800","2022-09-22T23:59:35","Observation","Ship Staff","Ship Staff Insp.","MOORING WINCH M3 & M4 MOORING WIRES TO BE RENEWED\nM3A/M3B/M4A & M4B","Deck - Mooring Machinery","Mooring","Equipment Related","","","","","Mooring Winch M3A/M3B/M4A/M4B wires renewed & greased","2022-10-02T23:59:35","","Completed","2022-09-29T23:59:35","No","No","No","Internal"]
[null,null,null,27265,29107,"27_Fri Oct 28 2022 17:53:16 GMT+0800","2022-09-27T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Mooring Winch M3 & M5 Abnormal noise while running Hydraulic Motor","Deck - Machinery","Mooring","Equipment Related","9.14","Medium","","","Troubleshooting is in progress.. Winch M5 no sound in last operation. M3 reported sound of hydraulic oil flow. Under observation. After close observation it was noted that sound heard is normal oil flow only. Issue stands closed.","2023-03-28T23:59:35","","Completed","2023-02-10T23:59:35","No","No","No","Internal"]
[null,null,null,27274,28806,"27_Fri Oct 28 2022 17:51:10 GMT+0800","2022-09-27T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Port & Stbd Provision Crane Luffing & Slewing limits not working","Deck - Machinery","General Appearance","Equipment Related","8.76","Medium","","","Both cranes limit switch eased up and working. ","2023-06-28T23:59:35","","Completed","2023-05-01T23:59:35","No","No","No","Internal"]
[null,null,null,27290,82297,"27_Sat Oct 15 2022 13:38:31 GMT+0800","2022-09-27T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","No.3 Port Manifold Valve CAV 21 found leaking","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","","","","","Seat Ring Renewed Size : 650A","2022-10-02T23:59:35","","Completed","2022-10-01T23:59:35","No","No","No","Internal"]
[null,null,null,27270,99683,"27_Fri Oct 28 2022 18:11:06 GMT+0800","2022-09-28T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Stbd Gangway Hoisting winch Platform bottom plate found wasted.","Deck - Machinery","Safety / LSA / FFA","Equipment Related","5.47","Medium","","","Soft Repairs done. Job to be carried out at next oppurtunity or during next docking.Job added in Refman. Removed as job has been added to REFMAN for drydock.","2022-12-27T23:59:35","","Completed","2022-09-28T23:59:35","No","No","No","Internal"]
[null,null,null,27277,45864,"27_Fri Oct 28 2022 18:17:05 GMT+0800","2022-09-30T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Port & Stbd MOB Brackets found wasted at few locations.","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.31","High","","","Soft Repairs carried out. Hot Work to be carried out at next oppurtunity or job to be caaried out during next docking.\nBracket renewed.","2023-03-28T23:59:35","","Completed","2023-01-03T23:59:35","No","No","No","Internal"]
[null,null,null,27291,47347,"27_Sat Oct 15 2022 13:41:15 GMT+0800","2022-10-05T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","Port Manifold Forward Vapour Manifold Valve leaking","Inert Gas","Cargo / Ballast Systems","Equipment Related","","","","","Seat Ring Renewed Size : 600 A.\nDeep pitting found on the bottom half of the valve body,cold repairs done","2022-10-16T23:59:35","","Completed","2022-10-11T23:59:35","No","No","No","Internal"]
[null,null,null,27283,65366,"27_Sat Oct 15 2022 13:43:55 GMT+0800","2022-10-06T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Few light brackets around accomodation area to be renewed","Elect. Mach. & Equip.","General Appearance","Equipment Related","11.11","Very High","","","Light brackets around accomodation areas renewed . ","2023-03-28T23:59:35","","Completed","2023-03-02T23:59:35","No","No","No","Internal"]
[null,null,null,27271,59452,"27_Fri Oct 28 2022 18:08:56 GMT+0800","2022-10-13T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Accomodation Railings found Wasted\nA Deck Port Side/B Deck Port Side/B Deck Stbd Side/Railing on Stbd side funnel deck adjacent to Waste oil tank vent/Stbd Pumproom Entrance adjacent to ODME Vent/Port Lifeboat Deck Adjacent to Embarkation light/Stbd Upper Deck Entrance adjacent to Fire Plan Box","Accommodation","Structural Condn. / WT integrity ","Equipment Related","11.5","Medium","","","Soft Repairs done. Job to be carried out at next oppurtunity or during next docking. Will do in ballast passage. Hot work of accommodation railing in progress. Vessel at Balboa anchorage.","2023-03-28T23:59:35","","Completed","2023-02-22T23:59:35","No","No","No","Internal"]
[null,null,null,27266,49439,"27_Fri Oct 28 2022 17:48:58 GMT+0800","2022-10-20T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Port Provision Crane Hoisting & Slewing Motor Gear oil to be renewed","Deck - Machinery","General Appearance","Equipment Related","8.76","Medium","","","Port Provision Crane Hoisting & Slewing Motor Gear oil to be renewed. Stbd provision crane gear oil renewed on 14-Feb-2023.","2023-03-29T23:59:35","","Completed","2023-03-13T23:59:35","No","No","No","Internal"]
[null,null,null,27269,68035,"27_Fri Oct 28 2022 17:54:45 GMT+0800","2022-10-20T23:59:35","Observation","Ship Staff","Ship Staff Insp.","VRCS Pump No.1 & No.2 - abnormal noise at times while pumps in use.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","11.4","Very High","","","Spares received, issue was observed with No 1 pump, same renwed, system working satisfactorily now.\n","2023-09-30T23:59:35","DLOT 230096","Completed","2023-09-28T23:59:35","No","No","No","Internal"]
[null,null,null,27275,25147,"27_Fri Oct 28 2022 17:57:02 GMT+0800","2022-10-20T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Stbd lifeboat davit harbour pin securing arrangements(fore and aft) found wasted.Port side only aft  found wasted\n","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.28","Very High","","","Cold work repairs completed on all 3 places. Job added in Refman. jOB CLOSED AS SAME WAS ADDED IN REFMAN","2022-12-27T23:59:35","","Completed","2022-10-23T23:59:35","No","No","No","Internal"]
[null,null,null,27285,93719,"27_Fri Oct 28 2022 17:47:11 GMT+0800","2022-10-20T23:59:35","Observation","Ship Staff","Ship Staff Insp.","2S COT Fwd COW Machine valve leaking","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.34","High","","","Valve to be renewed.target date amended. Job will be done at next opportunity.\nValve renewed","2022-12-27T23:59:35","","Completed","2022-10-22T23:59:35","No","No","No","Internal"]
[null,null,null,27267,98555,"27_Fri Oct 28 2022 17:59:00 GMT+0800","2022-10-21T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","Pin hole leak found on fire line elbow at port side boat deck","LSA / FFA","Safety / LSA / FFA","Equipment Related","11.7","High","","","Hot work carried out with office concurrence. New elbow welded. pressure tested. Found satisfactory.","2022-11-26T23:59:35","","Completed","2022-11-12T23:59:35","No","No","No","Internal"]
[null,null,null,27268,92374,"27_Fri Oct 28 2022 18:00:31 GMT+0800","2022-10-21T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Emg generator DO Tank vent and sounding pipe found wasted.","Deck - Pipe / Fittings","Emgcy. Systems","Equipment Related","11.7","High","","","Vent and sounding pipe renewed.","2023-03-27T23:59:35","","Completed","2023-03-22T23:59:35","No","No","No","Internal"]
[null,null,null,27272,61106,"27_Fri Oct 28 2022 18:02:24 GMT+0800","2022-10-21T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Gooseneck vent for Void space below Emergency generator found wasted.","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","Equipment Related","11.7","High","","","Gooseneck vent pipe renewed.","2023-03-27T23:59:35","","Completed","2023-03-22T23:59:35","No","No","No","Internal"]
[null,null,null,27273,60717,"27_Fri Oct 28 2022 18:04:37 GMT+0800","2022-10-21T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Emergency Generator Vent flaps found wasted","E/R - Pipes/ valves & fittings","Emgcy. Systems","Equipment Related","11.7","High","","","Flaps repaired.","2023-03-27T23:59:35","","Completed","2023-03-17T23:59:35","No","No","No","Internal"]
[null,null,null,27276,54367,"27_Fri Oct 28 2022 18:20:22 GMT+0800","2022-10-21T23:59:35","Observation","Ship Staff","Ship Staff Insp.","High Expansion Foam Tank Level Gauge Self Closing Spring Valve not holding.","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.40","Very High","","","The gauge glass was drained and the stuck valve was eased up. ","2023-03-27T23:59:35","DLOT220281 - HIGH EXPANSION FOAM TANK SPARES","Completed","2023-03-20T23:59:35","No","No","No","Internal"]
[null,null,null,27278,79601,"27_Fri Oct 28 2022 18:22:20 GMT+0800","2022-10-21T23:59:35","Observation","Ship Staff","Ship Staff Insp.","1 Fire man Walkie Talkie Battery safety locking pin broken. ","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.43","High","","","Requisition Raised.target date amended awaiting spare.\nSpares received and deployed.","2022-12-26T23:59:35","DLOT220233 - FIREMAN OUTFIT INTRINSICALLY SAFE WALKIE TALKIE\t","Completed","2022-12-18T23:59:35","No","No","No","Internal"]
[null,null,null,27279,30601,"27_Fri Oct 28 2022 18:24:56 GMT+0800","2022-10-21T23:59:35","Observation","Ship Staff","Ship Staff Insp.","1W PV Valve leaking","Cargo Mach.,Inert Gas","Cargo / Ballast Systems","Equipment Related","8.21","High","","","1W PV valve pressure seat renewed ","2023-03-27T23:59:35","DLOT220283 - CENTRE TANK- HIGH VELOCITY P/V RELIEF VALVE SPARES\nDLOT220282 - WING TANK-HIGH VELOCIT","Completed","2023-04-12T23:59:35","No","No","No","Internal"]
[null,null,null,27280,12398,"27_Fri Oct 28 2022 18:27:17 GMT+0800","2022-10-21T23:59:35","Observation","Ship Staff","Ship Staff Insp.","No.2 Port Manifold Valve Thrust Bearing Damaged.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.41","Medium","","","No.2 Port Manifold valve bearing replaced with No.4 Port Manifold.Damaged Bearing installed in No.4 Port Manifold - not to be used in discharge port.Requisition raised for new bearing.target date amended awaiting spare. Spare allegedly supplied as per supplier but same cannot be found onboard. Communication regarding this open.\nvessel awaiting abatement of heavy weather to carry out the job\nAll defective bearings renewed.","2023-03-27T23:59:35","DLOT220285 - Manifold Valve Thrust Ball Bearing","Completed","2022-12-31T23:59:35","No","No","No","Internal"]
[null,null,null,27281,56329,"27_Fri Oct 28 2022 18:29:33 GMT+0800","2022-10-21T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Few Mooring Winch Oil Level Sight Glass found opaque. ","Deck - Machinery","Mooring","Equipment Related","9.14","Medium","","","New Sight glass renewed on all mooring winches","2023-03-27T23:59:35","DLOT220240 - Mooring winch Spares","Completed","2023-02-28T23:59:35","No","No","No","Internal"]
[null,null,null,27282,52321,"27_Fri Oct 28 2022 18:37:55 GMT+0800","2022-10-21T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Steering Gear Room Rudder Angle Indicator Not working","Navigation - Others","Navigation","Equipment Related","","","","","The rudder angle indicator renewed","2023-06-14T23:59:35","DLOT230079 - RUDDER ANGLE INDICATOR ( STEERING R/M TYPE: VTR-5)","Completed","2023-06-09T23:59:35","No","No","No","Internal"]
[null,null,null,27286,55732,"27_Fri Oct 28 2022 18:34:38 GMT+0800","2022-10-21T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Accomodation Gas Detection System HC & Freon Sensors not working","Accommodation","General Appearance","Equipment Related","","","","","New cabinet received at Singapore in Jan 24, installed in place, follow up going on with Automation team. Both the sensors are connected in source mode, same configuration carried out for panel, working satisfactory.","2024-01-30T23:59:35","DLOT235063","Completed","2024-01-15T23:59:35","No","No","No","Internal"]
[null,null,null,29465,77416,"27_Wed Mar 08 2023 05:34:56 GMT+0800","2022-12-07T23:59:35","Observation,Non Conformity","Ship Staff","Nav Audit / Verification","WHEN ECDIS 1 (MONITORING - STBD SIDE) IS SET TO NIGHT OR DUSK MODE, FULL SCREEN BECOMES BLURRED AND GREEN, IN DAY MODE THERE IS AN EFFECT ON DISPLAY BUT STILL ALL INFORMATION IS VISIBLE AND READABLE.","Navigation - ECDIS","Navigation","Equipment Related","4.7","High","","","AWAITING SPARE","2023-07-07T23:59:35","DLOT 235015","Completed","2023-08-15T23:59:35","No","No","No","Internal","Spares have been supplied and monitor must be replaced soon."]
[null,null,null,29947,41859,"27_Thu Mar 30 2023 00:03:25 GMT+0800","2023-02-28T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Ballast fixed gas detection system gives failure alarm at times .","Miscellaneous","Cargo / Ballast Systems","Equipment Related","8.32","Low","","","Both pumps diaphragm changed and system put in use.","2023-06-29T23:59:35","DLOT 230052","Completed","2023-05-23T23:59:35","No","No","No","Internal"]
[null,null,null,29959,51844,"27_Fri Mar 24 2023 22:44:51 GMT+0800","2023-03-14T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ECR toilet flush not working. To rectify and clean.","Miscellaneous","Eng. / Strg. Comp.","Behaviour Based","11.13","Low","","","The toilet flushing valve was changed.","2023-03-31T23:59:35","","Completed","2023-03-26T23:59:35","No","No","No","Internal"]
[null,null,null,29960,45939,"27_Sat Mar 25 2023 21:56:53 GMT+0800","2023-03-14T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","D deck and E deck many of the cabin emergency light is not connected to the emergency power. ","Miscellaneous","General Appearance","Equipment Related","10.35","Very High","","","To check and modify.Required Lights changed in cabins and stores","2023-04-29T23:59:35","","Completed","2023-03-25T23:59:35","No","No","No","Internal"]
[null,null,null,29961,95260,"27_Fri Mar 24 2023 22:42:43 GMT+0800","2023-03-14T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Fixed chain block above ME intermediate shaft in rusted condition. To clean and grease.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.1","Medium","","","Chian blocks cleaned and greased. Tray painted.","2023-03-31T23:59:35","","Completed","2023-03-27T23:59:35","No","No","No","Internal"]
[null,null,null,29962,65077,"27_Sat Mar 25 2023 21:58:42 GMT+0800","2023-03-14T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","The cable for Engine room crane to renew. As the present one is in bad condition.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Cable renewed.","2023-04-03T23:59:35","","Completed",null,"No","No","No","Internal"]
[null,null,null,29964,96483,"27_Sat Mar 25 2023 22:02:25 GMT+0800","2023-03-14T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Leak of both service tank manhole door and quick closing valve to rectify.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.19","Very High","","","Both service tank manhole gaskets renewed.","2023-04-15T23:59:35","","Completed","2023-04-29T23:59:35","No","No","No","Internal"]
[null,null,null,29965,72068,"27_Fri Mar 24 2023 22:49:22 GMT+0800","2023-03-14T23:59:35","Observation","Ship Staff","Suptd. Insp.","Port side VRCS pump motor to overhaul as making abnormal noise. ","Miscellaneous","Cargo / Ballast Systems","Equipment Related","10.32","Very High","","","Motor was removed and checked. The sound is not from the motor.","2023-04-09T23:59:35","","Completed","2023-03-24T23:59:35","No","No","No","Internal"]
[null,null,null,29942,40486,"27_Sat Mar 25 2023 22:03:56 GMT+0800","2023-03-14T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Leaking valves of Air con units to renew. Vessel already supplied with new valve.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","","2023-06-29T23:59:35","","Completed","2023-08-15T23:59:35","No","No","No","Internal","I believe this is renewed alredy"]
[null,null,null,29943,76733,"27_Fri Mar 24 2023 22:07:35 GMT+0800","2023-03-14T23:59:35","Defect,Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ME Cyl CW inlet press gauge in ECR not operational. To renew","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.1","Medium","","","Trouble shooting done. The channel PCB in the DPU is malfunctioning. RO raised for the same.","2023-06-29T23:59:35","DLOT 230100","Completed","2023-08-15T23:59:35","No","No","No","Internal"]
[null,null,null,29944,89923,"27_Fri Mar 24 2023 22:47:12 GMT+0800","2023-03-14T23:59:35","Observation","Ship Staff","Suptd. Insp.","Rittle aircon to install for the EGB panel. Presently panel is kept in open condition,","E/R - Boiler","","Equipment Related","10.37","Medium","","","The spare air con available onboard ship is too big and cannot be fitted on the EGB panel.","2023-06-29T23:59:35","","Completed","2023-08-15T23:59:35","No","No","No","Internal"]
[null,null,null,29945,68019,"27_Wed Mar 29 2023 23:44:13 GMT+0800","2023-03-15T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Mast riser valve was found to be leaking . Temporary arrangements have been made . Awaiting requisition","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.19","High","","","MASTRISER VALVE OVERHAULED","2023-06-15T23:59:35","DLOT230090","Completed","2023-05-23T23:59:35","No","No","No","Internal"]
[null,null,null,29951,14674,"27_Thu Mar 30 2023 05:20:24 GMT+0800","2023-03-15T23:59:35","Non Conformity","Ship Staff","Ship Staff Insp.","AE No 3 unit no 1 and 2 exhaust temperature sensors malfunctioning.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Both sensors renewed.","2023-06-16T23:59:35","DLOT 230073","Completed","2023-06-14T23:59:35","No","No","No","Internal"]
[null,null,null,29466,62686,"27_Tue Mar 21 2023 07:36:13 GMT+0800","2023-03-17T23:59:35","Other","Ship Staff","Ship Staff Insp.","Portable gas equipment GX-8000 found malfunctioned","Miscellaneous","Cargo / Ballast Systems","Equipment Related","5.23","Very High","","","Spare sensors recieved and replaced . GX 8000 working satisfactory","2023-06-16T23:59:35","DLOT230081","Completed","2023-05-21T23:59:35","No","No","No","Internal"]
[null,null,null,29954,17293,"27_Sat Apr 15 2023 01:20:28 GMT+0800","2023-03-20T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","WMS sytem sampling pump motor not reaching required RPM causing reduced flow to the sensor","Elect. Mach. & Equip.","MARPOL Related","Equipment Related","10.30","High","","","Pump and motor renwed","2023-06-29T23:59:35","DLOT 230004","Completed","2023-05-29T23:59:35","No","No","No","Internal"]
[null,null,null,29963,73930,"27_Sun Apr 02 2023 21:40:16 GMT+0800","2023-03-24T23:59:35","Other","Ship Staff","Ship Staff Insp.","Few ballast level gauges erratic and not showing correct readinga","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.32","Low","","","Ballast valves level gauges calibrated . Working satisfactory","2023-06-23T23:59:35","","Completed","2023-04-27T23:59:35","No","No","No","Internal"]
[null,null,null,29952,50657,"27_Sat Apr 15 2023 01:12:29 GMT+0800","2023-04-03T23:59:35","Defect","Ship Staff","Ship Staff Insp.","AFT TRO unit optical sensor not working. PCB dmaged due to sea water leak. ","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.8","Medium","","","PCB renewed","2023-06-29T23:59:35","DLOT 230091","Completed","2023-05-23T23:59:35","No","No","No","Internal"]
[null,null,null,29953,53080,"27_Sat Apr 15 2023 01:15:23 GMT+0800","2023-04-05T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","ER blower fan no 1 motor burned.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Blower motor renewed","2023-06-29T23:59:35","DLOT 230094","Completed","2023-05-23T23:59:35","No","No","No","Internal"]
[null,null,null,29956,38399,"27_Sat Apr 15 2023 01:22:58 GMT+0800","2023-04-10T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","Dairy room fan not working","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.30","High","","","Motor renewed","2023-06-29T23:59:35","DLOT 230097","Completed","2023-05-23T23:59:35","No","No","No","Internal"]
[null,null,null,29957,76259,"27_Sat Apr 29 2023 00:02:58 GMT+0800","2023-04-26T23:59:35","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Fire/Foam monitor platforms on deck have RP gratings. These are to be repaced to metal gratings ","Deck - Pipe / Fittings","General Appearance","Equipment Related","5.38","High","","","Replaced all foam monitor platform gratings","2023-07-25T23:59:35","DLOT230107","Completed","2023-07-27T23:59:35","No","No","No","Internal"]
[null,null,null,29958,67165,"27_Sat Apr 29 2023 00:33:28 GMT+0800","2023-04-27T23:59:35","Defect","Ship Staff","Nav Audit / Verification","WHEN ECDIS 1 (MONITORING - STBD SIDE) IS SET TO NIGHT OR DUSK MODE, FULL SCREEN BECOMES BLURRED AND GREEN, IN DAY MODE THERE IS AN EFFECT ON DISPLAY BUT STILL ALL INFORMATION IS VISIBLE AND READABLE.","Navigation - ECDIS","Navigation","Equipment Related","4.7","High","","","Ecdis diaplay unit replaced with new one","2023-07-27T23:59:35","DLOT235015","Completed","2023-06-22T23:59:35","No","No","No","Internal"]
[null,null,null,30527,14742,"27_Sun Jun 18 2023 00:18:22 GMT+0800","2023-05-22T23:59:35","Observation","Ship Staff","Ship Staff Insp.","STBD provision crane vavle block leaking","Deck - Machinery","Eng. / Strg. Comp.","Equipment Related","10.2","Low","","","Leak rectified","2023-08-31T23:59:35","DLOT 230135","Completed","2023-07-28T23:59:35","No","No","No","Internal"]
[null,null,null,30529,70017,"27_Sat Jun 10 2023 08:48:18 GMT+0800","2023-06-06T23:59:35","Observation","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","Shore service report / job attendance sheet dated 08 Dec 2022 'AIR QUALITY TEST FOR BA COMPRESSOR  CARRIED OUT '. However test results were not available onboard","Documentation","Cert. & Docu.","Industry Issue","5.43","High","","","Test results were immediately received from the office and  have been received  and duly filed in ships filing system","2023-09-05T23:59:35","","Completed","2023-06-06T23:59:35","No","No","No","External"]
[null,null,null,30530,63088,"27_Sat Jun 10 2023 08:53:09 GMT+0800","2023-06-06T23:59:35","Observation","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","Port side after most cargo manifold valve , the pressure gauge manual valve operating handle was missing","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.41","Medium","","","The missing pressure gauge manual valve operating handle was immediately replaced with a new one","2023-09-05T23:59:35","","Completed","2023-06-06T23:59:35","No","No","No","External"]
[null,null,null,30526,65837,"27_Sun Jun 18 2023 00:14:29 GMT+0800","2023-06-11T23:59:35","Observation","Ship Staff","Ship Staff Insp.","ME RPM indicator in bridge wing having error.","Miscellaneous","Navigation","Equipment Related","10.1","Medium","","","Defective indicator renewed","2023-11-30T23:59:35","DLOT 230157","Completed","2023-11-09T23:59:35","No","No","No","Internal"]
[null,null,null,29949,66726,"27_Thu Mar 30 2023 05:07:15 GMT+0800","2023-06-15T23:59:35","Observation","Ship Staff","Ship Staff Insp.","ME unit No 6 temperature sensor malfunctioning","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Sensor renewed.","2023-09-15T23:59:35","DLOT 230075","Completed","2023-07-04T23:59:35","No","No","No","Internal"]
[null,null,null,29950,43875,"27_Thu Mar 30 2023 05:16:48 GMT+0800","2023-06-15T23:59:35","Observation","Ship Staff","Ship Staff Insp.","ME TC no 1 LO outlet temperatue sensor not working","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Sensor renewed","2023-09-15T23:59:35","DLOT 230075","Completed","2023-07-04T23:59:35","No","No","No","Internal","Will be supplied at the first convienent port"]
[null,null,null,31762,52275,"27_Sat Sep 16 2023 20:13:52 GMT+0800","2023-06-18T23:59:35","Defect","Ship Staff","Ship Staff Insp.","ME VIT cylinder leaking from the shaft seal","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Spares received at Singapore in Jan 24. wartsila shore technician replaced the old VIT actuator with new actuator, calibration carried out for VIT in coordination with Nabtesco. found satisfactory, Detailed report attached in servie reports.","2024-01-18T23:59:35","DLOT235052","Completed","2024-01-03T23:59:35","No","No","No","Internal"]
[null,null,null,31458,36896,"27_Thu Jun 22 2023 15:26:08 GMT+0800","2023-06-18T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Foam tank level not visible in the gauge glass.","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.40","Very High","","","FOAM TANK GAUGE GLASS OVERHAULED , SIGHT GLASS CLEANED AND PLACED BACK . FOAM TANK LEVEL NOW CLEARLY VISIBLE","2023-06-25T23:59:35","","Completed","2023-06-23T23:59:35","No","No","No","Internal"]
[null,null,null,31462,58870,"27_Wed Aug 16 2023 23:24:52 GMT+0800","2023-06-22T23:59:35","Defect","Ship Staff","Ship Staff Insp.","ME no.1 T/C exh. temperature found sensor defective.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Temperature sensor replaced with new spare.",null,"","Completed","2023-06-22T23:59:35","No","No","No","Internal"]
[null,null,null,29948,51309,"27_Thu Mar 30 2023 05:03:12 GMT+0800","2023-06-27T23:59:35","Observation","Ship Staff","Ship Staff Insp.","AE No 3 FO auto back was filter auto vent valve leaking.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Renewed the double nipple seals.","2023-09-29T23:59:35","DLOT 230087","Completed","2023-06-30T23:59:35","No","No","No","Internal"]
[null,null,null,31459,68527,"27_Wed Aug 16 2023 23:29:31 GMT+0800","2023-06-28T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Main Cooling Sea pump no. 1 found leaking from discharge pipe. ","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Pipe leakage rectified by welding in workshop. Intermediate piece fitted back and tried out, found satisfactory.",null,"","Completed","2023-06-29T23:59:35","No","No","No","Internal"]
[null,null,null,31463,73276,"27_Thu Aug 17 2023 00:02:09 GMT+0800","2023-06-29T23:59:35","Defect","Ship Staff","Ship Staff Insp.","FW hydrophore pump auto man switch found malfunctioning.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","","","","","FW hydrophore pump Auto man switch renewed .",null,"","Completed","2023-06-29T23:59:35","No","No","No","Internal"]
[null,null,null,29955,62830,"27_Sat Apr 15 2023 01:27:19 GMT+0800","2023-06-30T23:59:35","Observation","Ship Staff","Ship Staff Insp.","AE No 3 LO primming pump motor coupling worn out","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.30","High","","","AE No 3 LO primming pump motor coupling renewed.","2023-09-29T23:59:35","DLOT 230077","Completed","2023-07-02T23:59:35","No","No","No","Internal",""]
[null,null,null,31460,14725,"27_Wed Aug 16 2023 23:51:18 GMT+0800","2023-07-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Main Air Compressor no. 3 second stage gasket found leaking","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related","","","","","Gasket renewed with new spare",null,"","Completed","2023-07-01T23:59:35","No","No","No","Internal"]
[null,null,null,31461,99396,"27_Wed Aug 16 2023 23:56:32 GMT+0800","2023-07-02T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Aux engine no 3 turbo charger exhaust inlet temperature high","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Turbocharger removed from place and  cleaned . Nozzle ring cleaned .",null,"","Completed","2023-07-02T23:59:35","No","No","No","Internal"]
[null,null,null,31476,42751,"27_Thu Aug 17 2023 00:06:43 GMT+0800","2023-07-06T23:59:35","Defect","Ship Staff","Ship Staff Insp.","WMS pump No.2 Mechanical seal  leaking.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","","","","","WMS pump No.2 Mechanical seal renewed.",null,"","Completed","2023-07-06T23:59:35","No","No","No","Internal"]
[null,null,null,31464,64798,"27_Thu Aug 17 2023 00:10:37 GMT+0800","2023-07-10T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Aux Eng No.3, unit no 7 cylinder head exhaust gasket leaking.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","",""," cylinder head exhaust gasket renewed.",null,"","Completed","2023-07-10T23:59:35","No","No","No","Internal"]
[null,null,null,31454,71341,"27_Fri Jul 14 2023 16:10:58 GMT+0800","2023-07-11T23:59:35","Defect","Ship Staff","Ship Staff Insp.","APK tank level guage inoperational.","Miscellaneous","Cargo / Ballast Systems","Equipment Related","8.13","Medium","","","Troubleshooting carried out, gauge working satisfactorily","2023-09-11T23:59:35","","Completed","2023-09-11T23:59:35","No","No","No","Internal"]
[null,null,null,31455,82771,"27_Fri Jul 14 2023 16:15:21 GMT+0800","2023-07-11T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Issues with the BWTS system - FCV 1211 not working in auto or manual mode, can be operated only by handpump, GC raised for the same.","Miscellaneous","Cargo / Ballast Systems","Equipment Related","6.21","High","","","Faulty PCB replaced with new one, valve working remotelry now.","2023-10-12T23:59:35","","Completed","2023-10-01T23:59:35","No","No","No","Internal","Will be supplied at the first availabe opportunity"]
[null,null,null,31465,93055,"27_Thu Aug 17 2023 00:14:49 GMT+0800","2023-07-12T23:59:35","Defect","Ship Staff","Ship Staff Insp.","EGCS chamber  demister balls melted.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","All the melted demister balls removed and  gratings cleaned.",null,"","Completed","2023-07-12T23:59:35","No","No","No","Internal"]
[null,null,null,31466,31865,"27_Thu Aug 17 2023 00:18:06 GMT+0800","2023-07-19T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Aux Eng. No.2 FW pipe pipe o ring leaking","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","O ring renewed.",null,"","Completed","2023-07-19T23:59:35","No","No","No","Internal"]
[null,null,null,31474,64965,"27_Thu Aug 17 2023 00:23:18 GMT+0800","2023-07-24T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Starboard provision crane motor valve block  plug leaking.","Deck - Machinery","Cargo / Ballast Systems","Equipment Related","","","","","motor valve block  plug renewed",null,"","Completed","2023-07-24T23:59:35","No","No","No","Internal"]
[null,null,null,31467,39762,"27_Thu Aug 17 2023 00:26:53 GMT+0800","2023-07-25T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Windlass starboard control block plug leaking renewed","Deck - Machinery","Cargo / Ballast Systems","Equipment Related","","","",""," control block plug renewed",null,"","Completed","2023-07-25T23:59:35","No","No","No","Internal"]
[null,null,null,31468,11447,"27_Thu Aug 17 2023 00:29:09 GMT+0800","2023-07-26T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Aux Engine No.3 fuel oil inlet valve bonnet gasket leaking .","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","fuel oil inlet valve bonnet gasket renewed.",null,"","Completed","2023-07-26T23:59:35","No","No","No","Internal"]
[null,null,null,31475,99407,"27_Thu Aug 17 2023 00:32:30 GMT+0800","2023-07-27T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Aux Engine No.2  air cooler gasket leaking.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Air cooler gasket renewed",null,"","Completed","2023-07-27T23:59:35","No","No","No","Internal"]
[null,null,null,31473,64790,"27_Thu Aug 17 2023 00:34:39 GMT+0800","2023-07-28T23:59:35","Defect","Ship Staff","Ship Staff Insp.","ME unit no. 4 and unit no. 6 jacket water outlet pipe gasket leaking.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Jacket water outlet pipe gasket renewed.",null,"","Completed","2023-07-28T23:59:35","No","No","No","Internal"]
[null,null,null,31477,11177,"27_Thu Aug 17 2023 00:36:57 GMT+0800","2023-07-29T23:59:35","Defect","Ship Staff","Ship Staff Insp.","ME L O auto back wash filter ratchet malfunction..","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","L O auto back wash filter ratchet renewed",null,"","Completed","2023-07-29T23:59:35","No","No","No","Internal"]
[null,null,null,31469,58311,"27_Thu Aug 17 2023 00:39:35 GMT+0800","2023-07-30T23:59:35","Defect","Ship Staff","Ship Staff Insp.","AE no.3 T/C inlet temperature sensors malfunction.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","T/C inlet temperature sensors renewed.",null,"","Completed","2023-07-30T23:59:35","No","No","No","Internal"]
[null,null,null,31470,16572,"27_Thu Aug 17 2023 00:43:52 GMT+0800","2023-08-02T23:59:35","Defect","Ship Staff","Ship Staff Insp.","EGCS cooling sea water pump no.1 suction pipe found leaking .","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Pipe leakage rectified by welding in workshop. suction pipe fitted back and tried out, found satisfactory.",null,"","Completed","2023-08-02T23:59:35","No","No","No","Internal"]
[null,null,null,31456,25202,"27_Wed Aug 16 2023 16:58:48 GMT+0800","2023-08-05T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","Cargo tank gauging system WSU CPU is not booting up due to which there is no display of cargo tank level, ballast tank level and draft reading in CCR. Only cargo tank levels can be monitored in the standalone SCU unit.","Critical Equip.","Cargo / Ballast Systems","Equipment Related","8.12","Medium","","","New WSU received & readings coming in  Monitor. Technician attended in Singapore, readings displaying in CDU.","2023-12-30T23:59:35","DLOT235057 received","Completed","2024-01-03T23:59:35","No","No","No","Internal"]
[null,null,null,31472,38622,"27_Thu Aug 17 2023 00:51:04 GMT+0800","2023-08-10T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Pump room O2 sensor found malfunctioning. ","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","O2 sensor changed with new one and calibrated, found working well",null,"","Completed","2023-08-10T23:59:35","No","No","No","Internal"]
[null,null,null,31471,70718,"27_Thu Aug 17 2023 00:47:32 GMT+0800","2023-08-12T23:59:35","Defect","Ship Staff","Ship Staff Insp.","EGCS cooling sea water pump’s motor bearing found damaged .","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","","","","","Motor Bearing renewed.",null,"","Completed","2023-08-12T23:59:35","No","No","No","Internal"]
[null,null,null,31457,68231,"27_Wed Aug 16 2023 17:55:29 GMT+0800","2023-08-13T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Ship side railings at few places on poop deck found to be sheared off at weld seam due to corrosion","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","External Factors","11.3","Medium","","","Wasted section of railings cropped and fabricated new section fitted in place.","2024-01-31T23:59:35","","Completed","2024-01-18T23:59:35","No","No","No","Internal"]
[null,null,null,31746,61768,"0_Sat Sep 16 2023 10:26:13 GMT+0800","2023-09-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","ME # 1 T/C found surging at around 59~60% MCR with waste gate valve open around 18%.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Checked the operation of waste gate valve,  Found working satisfactory. Actuator removed Valve eased up.","2024-01-18T23:59:35","","Completed","2023-12-13T23:59:35","No","No","No","Internal"]
[null,null,null,31747,13259,"27_Sat Sep 16 2023 14:11:24 GMT+0800","2023-09-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","I/P converter for ME T/C waste gate valve not working","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","I/P converter checked by injecting current & found responding correspondingly, however the position of the damper was not changing accordingly. The problem is with control air piping leak, fitted with new copper piping. Made waste gate valve operational.","2023-11-30T23:59:35","","Completed","2023-12-10T23:59:35","No","No","No","Internal"]
[null,null,null,31748,90372,"0_Sat Sep 16 2023 14:14:11 GMT+0800","2023-09-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Exhaust leaking from ME # 1 T/C outlet bellow ","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","",""," ME # 1 T/C outlet bellow inspection carried out, found the bellow damaged. Shore technician attended at Singapore, replaced the cracked bellow with newly workshop fabricated bellow. Main engine tried out at full load, found satisfactory.","2024-01-30T23:59:35","","Completed","2024-01-03T23:59:35","No","No","No","Internal"]
[null,null,null,31749,19006,"0_Sat Sep 16 2023 14:16:00 GMT+0800","2023-09-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","ME exhaust gas leaking from EGB bypass damper","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Bellow inspected, found both bellow & gasket intact. Found the bolts loose, same were tightened. Also the lagging found to be completely damaged, same renewed.",null,"","Completed","2023-12-16T23:59:35","No","No","No","Internal"]
[null,null,null,31750,23803,"0_Sat Sep 16 2023 14:18:07 GMT+0800","2023-09-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","EGB soot blower system is not working in AUTO","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","Soot blower main air line valve actuator & one of the soot blower limit switch found malfunctioning, same renewed & system made operational .","2023-12-01T23:59:35","","Completed","2023-12-18T23:59:35","No","No","No","Internal"]
[null,null,null,31751,67151,"27_Sat Sep 16 2023 14:20:21 GMT+0800","2023-09-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","# 3 D/G FCU auto starting of pumps is taking place even when the FO pressure is normal due to malfunction of the auto c/o pressure switch.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","All the connections removed & put back as no abnormality in the control circuit found. Suspect some loose cable connection. Now the pumps changeover is not taking place, working satisfactory.","2023-11-30T23:59:35","","Completed","2023-10-21T23:59:35","No","No","No","Internal"]
[null,null,null,31752,23674,"27_Sat Sep 16 2023 14:23:05 GMT+0800","2023-09-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","EGCS WMS02 effluent sampling pump not working","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","Same replaced with spare new pump. old pump overhauled, motor overhauled seals changed and kept standby for future use.","2023-11-30T23:59:35","","Completed","2023-11-18T23:59:35","No","No","No","Internal"]
[null,null,null,31753,71052,"27_Sat Sep 16 2023 19:44:54 GMT+0800","2023-09-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Control air pressure reducing valve malfunctioning","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","The pressure reducing valve outlet valve is not holding, also the root valve of the control air line is connected to the D/G start air line making it difficult to remove the valve. Spare reducing valve received at Singapore in jan 24. Main engine to be in stopped condition to carry out this job. Valve replaced with new spare, found satisfactory in operation.","2024-04-30T23:59:35","DLOT230301 ","Completed","2024-02-10T23:59:35","No","No","No","Internal"]
[null,null,null,31754,93953,"27_Sat Sep 16 2023 19:46:56 GMT+0800","2023-09-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","# 1 LT cooler SW outlet valve not holding","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","same replaced with spare new valve.","2023-11-30T23:59:35","","Completed","2023-11-01T23:59:35","No","No","No","Internal"]
[null,null,null,31755,42670,"0_Sat Sep 16 2023 19:48:55 GMT+0800","2023-09-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","# 1 LT cooler backwash line SW inlet valve body has a pin hole","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Same replaced with spare new valve.","2023-11-30T23:59:35","","Completed","2023-11-01T23:59:35","No","No","No","Internal"]
[null,null,null,31756,13418,"0_Sat Sep 16 2023 19:50:17 GMT+0800","2023-09-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","# 2 LT cooler SW outlet valve body holed, same needs renewal","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Same replaced with spare new valve.",null,"","Completed","2023-11-01T23:59:35","No","No","No","Internal"]
[null,null,null,31757,31796,"0_Sat Sep 16 2023 14:12:36 GMT+0800","2023-09-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","I/P converter for ME EGB inlet damper actuator not working","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","I/P converter checked by injecting current & found responding correspondingly, however the position of the damper was not changing accordingly. The problem was with control air piping, same connected to the spare piping given. Damper found working satisfactory.","2023-11-30T23:59:35","","Completed","2023-11-01T23:59:35","No","No","No","Internal"]
[null,null,null,31758,43780,"0_Sat Sep 16 2023 19:51:42 GMT+0800","2023-09-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","# 2 LT cooler SW inlet pipe leaking through pin hole","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Same rectified by hot work in ER workshop","2023-11-30T23:59:35","","Completed","2023-11-01T23:59:35","No","No","No","Internal"]
[null,null,null,31765,40627,"27_Sun Sep 17 2023 07:12:05 GMT+0800","2023-09-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Bunker tank void space (p) - oil leak found. One gasket on the LSMGO line found damaged","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Flange bolts found slack, tightening carried out. No leak observed.","2023-11-30T23:59:35","","Completed","2023-11-23T23:59:35","No","No","No","Internal"]
[null,null,null,31780,21742,"27_Sat Sep 16 2023 10:11:41 GMT+0800","2023-09-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","ME bypass damper found malfunctioning.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","ME bypass damper solenoid valve found stuck, same o'hauled & made operational.","2023-09-30T23:59:35","","Completed","2023-09-04T23:59:35","No","No","No","Internal"]
[null,null,null,31781,24006,"0_Sat Sep 16 2023 10:13:34 GMT+0800","2023-09-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","# 3 D/G bypass damper found malfunctioning","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","# 3 D/G bypass damper solenoid valve replaced, also limit switch setting done. Bypass damper made operational in AUTO.","2023-09-30T23:59:35","","Completed","2023-09-06T23:59:35","No","No","No","Internal"]
[null,null,null,31784,52380,"0_Sat Sep 16 2023 08:54:13 GMT+0800","2023-09-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","# 2 Boiler water circulating pump found leaking from the shaft seal.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","","","","","# 2 Boiler water circulating pump shaft seal renewed.","2023-09-15T23:59:35","","Completed","2023-09-01T23:59:35","No","No","No","Internal"]
[null,null,null,31787,49368,"0_Sun Sep 17 2023 07:19:31 GMT+0800","2023-09-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","# 2 D/G rpm indicator panel - WIP 10 found malfunctioning","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","# 2 D/G rpm indicator panel - WIP 10 replaced with new spare, made operational.","2023-11-30T23:59:35","","Completed","2023-09-14T23:59:35","No","No","No","Internal"]
[null,null,null,31788,34963,"0_Sun Sep 17 2023 07:22:41 GMT+0800","2023-09-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","# 1 D/G selection knob control panel WCP-10 found malfunctioning","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","# 1 D/G selection knob control panel WCP-10 replaced with a new spare, made operational.","2023-11-30T23:59:35","","Completed","2023-09-14T23:59:35","No","No","No","Internal"]
[null,null,null,31791,43040,"27_Sat Sep 16 2023 10:03:28 GMT+0800","2023-09-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","E/R workshop AC was not operational since long time","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","E/R workshop AC replaced with new spare and made operational","2023-09-30T23:59:35","","Completed","2023-09-04T23:59:35","No","No","No","Internal"]
[null,null,null,31785,37209,"0_Sat Sep 16 2023 08:56:51 GMT+0800","2023-09-02T23:59:35","Defect","Ship Staff","Ship Staff Insp.","BNWAS stbd side bell was not operating.","Navigation - VDR / BNWAS","Navigation","Equipment Related","","","","","Same checked and found terminal module channel not giving output. Used spare channel and tested the bell, working satisafctory.","2023-09-15T23:59:35","","Completed","2023-09-02T23:59:35","No","No","No","Internal"]
[null,null,null,31774,50758,"27_Wed Sep 13 2023 16:39:22 GMT+0800","2023-09-04T23:59:35","Defect","Ship Staff","Ship Staff Insp.","EGCS cooling sea water pump no.3 discharge side pipe found leaking.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","EGCS cooling sea water pump no.3 discharge side pipe removed from location for leak rectification. Welding carried out in engine room workshop and pipe was fixed back in place.","2023-09-15T23:59:35","","Completed","2023-09-07T23:59:35","No","No","No","Internal"]
[null,null,null,31760,53209,"0_Sat Sep 16 2023 19:55:31 GMT+0800","2023-09-05T23:59:35","Defect","Ship Staff","Ship Staff Insp.","ME FO viscosity controller malfunctioning","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","Sensor removed, pendulum cleaned & fitted back, found working satisfactory.","2023-11-30T23:59:35","","Completed","2023-11-01T23:59:35","No","No","No","Internal"]
[null,null,null,31761,28118,"0_Sat Sep 16 2023 19:56:44 GMT+0800","2023-09-05T23:59:35","Defect","Ship Staff","Ship Staff Insp.","# 3 D/G viscosity controller malfunctioning","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","Viscosity sensor pendulum cover sleeve found dislocated from its position, sensor  cleaned & fitted back in place. Found working satisfactory.","2023-11-30T23:59:35","","Completed","2023-11-10T23:59:35","No","No","No","Internal"]
[null,null,null,31766,24083,"27_Sun Sep 17 2023 07:41:05 GMT+0800","2023-09-09T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Inventory of Crane hoses to be verified and updated and damaged O rings to be replaced and kept ready for emergency use.","Deck - Machinery","Cargo / Ballast Systems","Equipment Related","","","","","Inventory taken and updated","2023-10-09T23:59:35","","Completed","2023-11-14T23:59:35","No","No","No","Internal"]
[null,null,null,31768,58295,"0_Sun Sep 17 2023 07:50:43 GMT+0800","2023-09-09T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Air ejector cooling sea water valve leak to rectify.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Air ejector SW inlet valve renewed, outlet valve fitted with old body.","2023-11-09T23:59:35","","Completed","2023-11-04T23:59:35","No","No","No","Internal"]
[null,null,null,31769,88286,"0_Sun Sep 17 2023 07:52:45 GMT+0800","2023-09-09T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","OPEN, SHUT indication in Engine room blower faded, to be stenciled.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","OPEN SHUT Indication stenciled on all Engine room blowers.","2023-09-23T23:59:35","","Completed","2023-09-21T23:59:35","No","No","No","Internal"]
[null,null,null,31770,56996,"0_Sun Sep 17 2023 07:46:08 GMT+0800","2023-09-09T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Drums in steering flat to be secured with 3 nos of gripes, with wooden plank or rubber material between the drum and wire rope.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","Drums in steering flat arranged and secured with wooden material in between drum and wire ropes.","2023-09-24T23:59:35","","Completed","2023-09-22T23:59:35","No","No","No","Internal"]
[null,null,null,31782,87194,"27_Sat Sep 16 2023 10:18:41 GMT+0800","2023-09-09T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Aux Eng no.2, unit no.1 exhaust temperature high alarm","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Cylinder head replaced with o'hauled one. Exhaust temperature found within normal range. ","2023-09-12T23:59:35","","Completed","2023-09-11T23:59:35","No","No","No","Internal"]
[null,null,null,31792,95094,"27_Sun Sep 17 2023 07:36:16 GMT+0800","2023-09-09T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Port side Lifeboat sprinkler system suction valve to ease up.","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","Port side Lifeboat sprinkler system suction valve eased up.","2023-09-16T23:59:35","","Completed","2023-09-12T23:59:35","No","No","No","Internal"]
[null,null,null,31793,54375,"0_Sun Sep 17 2023 07:38:01 GMT+0800","2023-09-09T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Foam tank to top up and minimum level to be marked with arrow.","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","Foam tank topped up and minimum level marked with arrow","2023-09-16T23:59:35","","Completed","2023-09-13T23:59:35","No","No","No","Internal"]
[null,null,null,31796,36698,"0_Sun Sep 17 2023 07:45:03 GMT+0800","2023-09-09T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Fwd deck machinery hydraulic cooler leak to rectify.","Deck - Mooring Machinery","Mooring","Equipment Related","","","","","Fwd deck machinery hydraulic cooler leak rectified.","2023-09-29T23:59:35","","Completed","2023-09-14T23:59:35","No","No","No","Internal"]
[null,null,null,31797,55069,"0_Sun Sep 17 2023 07:49:14 GMT+0800","2023-09-09T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","M.E. fuel valve return line to be secured with clamps","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","M.E. fuel valve return line secured with clamps.","2023-09-17T23:59:35","","Completed","2023-09-17T23:59:35","No","No","No","Internal"]
[null,null,null,31798,65187,"0_Sun Sep 17 2023 07:43:16 GMT+0800","2023-09-09T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Deck seal overboard valve leak in pumproom to rectify.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","","","","","Leak rectified","2023-10-09T23:59:35","","Completed","2023-09-15T23:59:35","No","No","No","Internal"]
[null,null,null,31771,84447,"27_Sun Sep 17 2023 19:58:16 GMT+0800","2023-09-10T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Exhaust gas leaking from EGCS ME bypass damper inlet bellow","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","EGCS bypass damper inlet bellow inspected, found the gasket & bellow intact. Bolts found loose, same were tightened. ","2023-12-10T23:59:35","","Completed","2023-12-11T23:59:35","No","No","No","Internal"]
[null,null,null,31772,63860,"0_Sun Sep 17 2023 20:00:21 GMT+0800","2023-09-10T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Refrigerant gas leaking from Fridge system ","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Shore team carried out leak test, found leak at copper pipe near at lobby, leak arrested. system tried out found satisfactory.","2024-01-30T23:59:35","","Completed","2024-01-03T23:59:35","No","No","No","Internal"]
[null,null,null,31786,86400,"27_Sun Sep 17 2023 07:07:50 GMT+0800","2023-09-10T23:59:35","Defect","Ship Staff","Ship Staff Insp.","FWG suction line pipe found leaking","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Pipe fabricated & fitted back","2023-11-30T23:59:35","","Completed",null,"No","No","No","Internal"]
[null,null,null,32578,64008,"0_Mon Nov 20 2023 05:41:10 GMT+0800","2023-09-10T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Air ejector SW outlet valve leaking from valve body.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Spares received onboard at Singapore in jan 24. Valve replaced with new spare, found satisfactory in operation.","2024-04-30T23:59:35","DLOT230274","Completed","2024-02-21T23:59:35","No","No","No","Internal"]
[null,null,null,31775,40066,"27_Thu Sep 14 2023 08:50:14 GMT+0800","2023-09-11T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Port side Lifeboat sprinkler system suction valve to ease up.","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.28","Very High","","","Both lifeboat sprinkler valves eased up and now operating freely.","2023-12-10T23:59:35","","Completed","2023-09-13T23:59:35","No","No","No","Internal"]
[null,null,null,31776,60219,"0_Thu Sep 14 2023 08:51:52 GMT+0800","2023-09-11T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Foam tank to top up and minimum level to be marked with arrow.","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.35","Medium","","","Foam tank topped up ","2023-12-10T23:59:35","","Completed","2023-09-13T23:59:35","No","No","No","Internal"]
[null,null,null,31777,90784,"0_Thu Sep 14 2023 08:58:44 GMT+0800","2023-09-11T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Fwd deck machinery hydraulic cooler leak to rectify.","Deck - Mooring Machinery","Mooring","Equipment Related","11.4","Very High","","","Repairs on cooler pipe carried out. Tested & no leaks observed.","2023-12-10T23:59:35","","Completed","2023-09-14T23:59:35","No","No","No","Internal"]
[null,null,null,31778,93565,"0_Thu Sep 14 2023 08:56:58 GMT+0800","2023-09-11T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Deck seal overboard valve leak in pumproom to rectify.","Miscellaneous","Structural Condn. / WT integrity ","Equipment Related","11.4","Very High","","","Found small leak from upper valve body. Bolts tightened & leak stopped.\n","2023-12-10T23:59:35","","Completed","2023-09-14T23:59:35","No","No","No","Internal"]
[null,null,null,31743,85976,"0_Thu Sep 14 2023 08:54:13 GMT+0800","2023-09-11T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Inventory of Crane hoses to be verified and updated and damaged O rings to be replaced and kept ready for emergency use.","Miscellaneous","General Appearance","Inappropriate Procedure","8.50","Medium","","","Inventory updated and RO raised for missing hoses","2023-12-10T23:59:35","","Completed","2023-11-30T23:59:35","No","No","No","Internal"]
[null,null,null,31763,80697,"27_Sat Sep 16 2023 21:19:47 GMT+0800","2023-09-12T23:59:35","Defect","Ship Staff","Ship Staff Insp.","FWG salinometer malfunctioning","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Spares received at Singapore in Jan 24, salinometer replaced with new one, found satisfactory.","2024-01-30T23:59:35","DLOT230225 ","Completed","2024-01-09T23:59:35","No","No","No","Internal"]
[null,null,null,31764,73384,"27_Sat Sep 16 2023 21:21:13 GMT+0800","2023-09-12T23:59:35","Defect","Ship Staff","Ship Staff Insp.","FWG flowmeter not working","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Spares received, Flowmeter is replaced with new spare.","2024-01-30T23:59:35","DLOT230225 ","Completed","2024-01-11T23:59:35","No","No","No","Internal"]
[null,null,null,31783,15894,"0_Sat Sep 16 2023 10:20:49 GMT+0800","2023-09-12T23:59:35","Defect","Ship Staff","Ship Staff Insp.","# 2 D/G T/C bank A inlet bellow found cracked ","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","# 2 D/G T/C bank A inlet bellow replaced with new spare ",null,"","Completed","2023-09-12T23:59:35","No","No","No","Internal"]
[null,null,null,31779,65631,"0_Sat Sep 16 2023 08:51:26 GMT+0800","2023-09-14T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Air line pressure reducing valve(30 ~ 7 K) found malfunctioning ","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Pressure reducing valve o'hauled, seal ring replaced with teflon seal ring. Working satisfactory.","2023-09-30T23:59:35","","Completed","2023-09-14T23:59:35","No","No","No","Internal"]
[null,null,null,31789,58167,"0_Sun Sep 17 2023 07:25:08 GMT+0800","2023-09-14T23:59:35","Defect","Ship Staff","Ship Staff Insp.","# 1 D/G Fuel rack stop position limit switch found not working","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","# 1 D/G Fuel rack stop position limit switch replaced with new spare, made operational.","2023-11-30T23:59:35","","Completed","2023-09-14T23:59:35","No","No","No","Internal"]
[null,null,null,31745,15295,"0_Sat Sep 16 2023 08:47:53 GMT+0800","2023-09-15T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Service air compressor tripping on LO high temp alarm, need to renew LO cooler","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related","","","","","LO cooler received & replaced the old one. Made Service air compressor operational.","2023-12-15T23:59:35","RO -DLOT230224  ","Completed","2023-12-11T23:59:35","No","No","No","Internal"]
[null,null,null,31790,61750,"0_Sun Sep 17 2023 07:28:08 GMT+0800","2023-09-15T23:59:35","Defect","Ship Staff","Ship Staff Insp.","# 1 D/G LT cooling water pressure transmitter found not working.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","# 1 D/G LT cooling water pressure transmitter replaced with new spare","2023-11-30T23:59:35","","Completed","2023-09-15T23:59:35","No","No","No","Internal"]
[null,null,null,31794,91167,"27_Sun Sep 17 2023 08:44:02 GMT+0800","2023-09-15T23:59:35","Defect","Ship Staff","Ship Staff Insp.","# 2 Main cooling sea water pump root valve for mechanical seal cooling found broken.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","","","","","Same renewed with stainless steel valve.","2023-09-20T23:59:35","","Completed","2023-09-16T23:59:35","No","No","No","Internal"]
[null,null,null,31795,70261,"0_Sun Sep 17 2023 08:48:06 GMT+0800","2023-09-16T23:59:35","Defect","Ship Staff","Suptd. Insp.","E/R # 3 blower flap one section bolts found broken ","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","E/R # 3 blower flap broken section bolts renewed.","2023-09-16T23:59:35","","Completed","2023-09-16T23:59:35","No","No","No","Internal"]
[null,null,null,32572,48392,"27_Mon Nov 20 2023 05:26:51 GMT+0800","2023-09-16T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Service air compressor tripping on LO high temperature due to dirty LO cooler","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related","","","","","LO cooler renewed & service air compressor made operational.","2023-12-16T23:59:35","","Completed","2023-12-11T23:59:35","No","No","No","Internal"]
[null,null,null,32587,88632,"27_Sat Nov 18 2023 08:35:39 GMT+0800","2023-09-16T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Engine room blower fan no.3 flap fell out from place due to corroded bolts.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","",""," Same fitted back with new bolts.","2023-12-16T23:59:35","","Completed","2023-09-16T23:59:35","No","No","No","Internal"]
[null,null,null,32588,93352,"27_Sat Nov 18 2023 08:30:22 GMT+0800","2023-09-16T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Aux engine no.1, LT water pressure transmitter found malfunctioning.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Aux engine no.1, LT water pressure transmitter renewed ","2023-09-30T23:59:35","","Completed","2023-11-16T23:59:35","No","No","No","Internal"]
[null,null,null,32590,43872,"27_Sat Nov 18 2023 08:44:24 GMT+0800","2023-09-16T23:59:35","Defect","Ship Staff","Ship Staff Insp.","DG#1 LT pressure transmitter found not working.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","same renewed.","2023-12-15T23:59:35","","Completed","2023-09-16T23:59:35","No","No","No","Internal"]
[null,null,null,32589,77231,"27_Sat Nov 18 2023 08:41:59 GMT+0800","2023-09-17T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Stop position limit switch for DG#1 found not operational.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","same renewed","2023-12-16T23:59:35","","Completed","2023-09-17T23:59:35","No","No","No","Internal"]
[null,null,null,32591,69560,"27_Sat Nov 18 2023 08:53:58 GMT+0800","2023-09-18T23:59:35","Defect","Ship Staff","Ship Staff Insp.","EGCS cooling sea water pump no.3 suction side found leaking. ","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","","","","","same removed from place, leak rectified and put back in the place.","2023-12-17T23:59:35","","Completed","2023-09-18T23:59:35","No","No","No","Internal"]
[null,null,null,32626,24206,"27_Sun Nov 19 2023 11:15:13 GMT+0800","2023-09-18T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Stern light both main and sub got fused same day on inspection found water went inside and holders were in bad condition.","Navigation - Others","Eng. / Strg. Comp.","Equipment Related","","","","","renewed light and junction box.","2023-12-18T23:59:35","","Completed","2023-09-18T23:59:35","No","No","No","Internal"]
[null,null,null,32592,36183,"0_Sat Nov 18 2023 08:56:38 GMT+0800","2023-09-19T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Deck seal pump no.1 discharge pipe side found leaking. ","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","","","","","pipe removed from place, leak rectified and put back in place.","2023-12-18T23:59:35","","Completed","2023-09-19T23:59:35","No","No","No","Internal"]
[null,null,null,32627,20439,"27_Sun Nov 19 2023 11:21:26 GMT+0800","2023-09-19T23:59:35","Defect","Ship Staff","Ship Staff Insp.","In accommodation gas detection system found that HC sensor is connected to channel 2, but display is not lit. the display is coming when entered in the calibration mode.  Even after swapping sensors no display was observed in channel 2. ","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","Suspect channel 2 is not programmed or defective","2023-12-18T23:59:35","","Completed","2023-09-19T23:59:35","No","No","No","Internal"]
[null,null,null,32593,91466,"27_Sat Nov 18 2023 08:59:01 GMT+0800","2023-09-20T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Key operator for Aux. boiler Auto and Manuel selection for No.1 and No.2. found damaged.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","same renewed.","2023-12-19T23:59:35","","Completed","2023-09-20T23:59:35","No","No","No","Internal"]
[null,null,null,32594,33494,"27_Sat Nov 18 2023 09:00:46 GMT+0800","2023-09-20T23:59:35","Defect","Ship Staff","Ship Staff Insp.","solenoid valve for No.2 Boiler pneumatic actuators found not operating ","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","solenoid valve renewed.","2023-12-20T23:59:35","","Completed","2023-09-20T23:59:35","No","No","No","Internal"]
[null,null,null,32595,85017,"27_Sat Nov 18 2023 09:03:13 GMT+0800","2023-09-21T23:59:35","Defect","Ship Staff","Ship Staff Insp.","WMS 002 was not showing flow checked the same and found that the strainer was chocked.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","Same cleaned and put back.","2023-12-17T23:59:35","","Completed","2023-09-21T23:59:35","No","No","No","Internal"]
[null,null,null,32628,18767,"27_Sun Nov 19 2023 11:25:04 GMT+0800","2023-09-21T23:59:35","Defect","Ship Staff","Ship Staff Insp.","VECS is found not giving the low pressure alarm when the line pressure is below 10 and it is giving low pressure alarm when line pressure is above 10.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","",""," Same rectified by changing alarm set points as per maker manual.","2023-12-19T23:59:35","","Completed","2023-09-21T23:59:35","No","No","No","Internal"]
[null,null,null,32600,85203,"27_Sat Nov 18 2023 09:07:37 GMT+0800","2023-09-22T23:59:35","Defect","Ship Staff","Ship Staff Insp.","freon sensor for accommodation found not working.","Accommodation","Eng. / Strg. Comp.","Equipment Related","","","","","same renewed.","2023-12-22T23:59:35","","Completed","2023-09-22T23:59:35","No","No","No","Internal"]
[null,null,null,32596,63387,"27_Sat Nov 18 2023 09:13:23 GMT+0800","2023-09-23T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Refer compressor pully was wobbling and belt was slipped out found that shaft and key got damaged.","Accommodation","Eng. / Strg. Comp.","Equipment Related","","","","","Installed spare refer compressor","2023-12-23T23:59:35","","Completed","2023-09-23T23:59:35","No","No","No","Internal"]
[null,null,null,32601,70840,"27_Sat Nov 18 2023 09:10:29 GMT+0800","2023-09-23T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Emergency DG battery chargers one relay found faulty.","Elect. Mach. & Equip.","Emgcy. Systems","Equipment Related","","","","","relay renewed.","2023-12-23T23:59:35","","Completed","2023-09-23T23:59:35","No","No","No","Internal"]
[null,null,null,32629,38409,"0_Sun Nov 19 2023 11:28:04 GMT+0800","2023-09-23T23:59:35","Defect","Ship Staff","Ship Staff Insp.","hyper mist system was giving loop earth fault alarm, found  that earth fault was coming form heat and smoke sensor above DG#3 ","LSA / FFA","Emgcy. Systems","Equipment Related","","","","","renewed the sensor and tried out the alarm found working satisfactory.","2023-12-19T23:59:35","","Completed","2023-09-23T23:59:35","No","No","No","Internal"]
[null,null,null,32552,98999,"27_Tue Sep 26 2023 07:57:02 GMT+0800","2023-09-24T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Few valve indicators in CCR panel not functioning properly.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.11","Medium","","","DLOT230231 Received. Installation in progress. Valve indicators in hydraulic room replaced with overhauled/new spares. Found satisfactory in operation.","2024-01-31T23:59:35","DLOT230231","Completed","2024-01-10T23:59:35","No","No","No","Internal"]
[null,null,null,32597,97322,"27_Sat Nov 18 2023 09:16:30 GMT+0800","2023-09-24T23:59:35","Defect","Ship Staff","Ship Staff Insp.","WMS 001 flow was not showing found that the strainer and de-bubbler got chocked","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","same cleaned and put back now working satisfactory","2023-12-24T23:59:35","","Completed","2023-09-24T23:59:35","No","No","No","Internal"]
[null,null,null,32604,21291,"27_Sat Nov 18 2023 09:18:54 GMT+0800","2023-09-24T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Hyper mist MCP for ME found broken","LSA / FFA","Emgcy. Systems","Equipment Related","","","","","renewed the same with spare and tried out the MCP. Working satisfactory.","2023-12-24T23:59:35","","Completed","2023-09-24T23:59:35","No","No","No","Internal"]
[null,null,null,32598,94085,"27_Sat Nov 18 2023 09:24:42 GMT+0800","2023-09-26T23:59:35","Defect","Ship Staff","Ship Staff Insp.","EGCS room dampers found not working.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","maintenance carried out rusting removed, painted  and dampers tried out for operation. found satisfactory.","2023-12-26T23:59:35","","Completed","2023-09-26T23:59:35","No","No","No","Internal"]
[null,null,null,32599,50648,"27_Sat Nov 18 2023 09:27:18 GMT+0800","2023-09-26T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Scrubber entrance light fitting found broken due to corrosion.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","same renewed ","2023-12-26T23:59:35","","Completed","2023-09-26T23:59:35","No","No","No","Internal"]
[null,null,null,32608,77454,"27_Sat Nov 18 2023 09:30:28 GMT+0800","2023-09-27T23:59:35","Defect","Ship Staff","Ship Staff Insp.","In Aux. blower no 1  found that one cable going to motor is burnt and the contactor is not making contact.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Renewed the contactors with spare.","2023-12-27T23:59:35","","Completed","2023-09-27T23:59:35","No","No","No","Internal"]
[null,null,null,32632,82909,"0_Sun Nov 19 2023 11:33:27 GMT+0800","2023-09-27T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Life Boat winch handle limit switch inspection carried out found Port side limit switch stuck.","LSA / FFA","Emgcy. Systems","Equipment Related","","","",""," Eased up the limit switch and now it is working smoothly.","2023-12-27T23:59:35","","Completed","2023-09-27T23:59:35","No","No","No","Internal"]
[null,null,null,32602,42456,"27_Sat Nov 18 2023 09:32:52 GMT+0800","2023-09-28T23:59:35","Defect","Ship Staff","Ship Staff Insp.","ALDIS lamp found not working. same checked and found that the cable was broken. ","Elect. Mach. & Equip.","Navigation","Equipment Related","","","","","Rectified and checked working satisfactory.","2023-12-28T23:59:35","","Completed","2023-09-28T23:59:35","No","No","No","Internal"]
[null,null,null,32636,19435,"0_Sun Nov 19 2023 11:37:08 GMT+0800","2023-09-29T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Changed Deep draft light fitting on main mast found damaged . Checked the light which was lit and found that relay was faulty.","Elect. Mach. & Equip.","Navigation","Equipment Related","","","","","renewed with new fitting and tried out again alarm, found satisfactory.  faulty relay renewed with new and tried out working satisfactory.","2023-12-28T23:59:35","","Completed","2023-09-29T23:59:35","No","No","No","Internal"]
[null,null,null,32553,83024,"27_Fri Oct 06 2023 08:11:59 GMT+0800","2023-10-02T23:59:35","Observation","Ship Staff","Ship Staff Insp.","One of the CCr window glass is shattered, need to renew","Miscellaneous","General Appearance","Equipment Related","11.6","Medium","","","New glass installed.","2024-03-30T23:59:35","DLOT230226","Completed","2024-01-23T23:59:35","No","No","No","Internal"]
[null,null,null,32554,31955,"0_Fri Oct 06 2023 08:14:41 GMT+0800","2023-10-02T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Poor condition of VRCS system flanges and leak from one of the T block joint","Miscellaneous","Cargo / Ballast Systems","Equipment Related","11.4","Very High","","","Leaking section opened and o-ring renewed. Presently leaking is stopped. ","2024-01-01T23:59:35","","Completed","2023-11-20T23:59:35","No","No","No","Internal"]
[null,null,null,32603,14880,"27_Sat Nov 18 2023 09:36:18 GMT+0800","2023-10-02T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Boiler water circulating pump #1  coupling found damaged.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","","","","","coupling renewed and pump tried out. found working satisfactorily. ","2024-01-02T23:59:35","","Completed","2023-10-02T23:59:35","No","No","No","Internal"]
[null,null,null,32613,19144,"27_Sat Nov 18 2023 09:38:31 GMT+0800","2023-10-02T23:59:35","Defect","Ship Staff","Ship Staff Insp.","BWTS FCV 1211 PCB found not working.\t\t\t\t\t\t\t","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","same renewed and tried out working satisfactory.\t","2024-01-02T23:59:35","","Completed","2023-10-02T23:59:35","No","No","No","Internal"]
[null,null,null,32640,43915,"0_Sun Nov 19 2023 11:40:24 GMT+0800","2023-10-02T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Shaft grounding device -  checked the cable condition and the terminals found rusted. \t\t\t\t\t\t\t\t\t\t\t\t\t\t\t\t\t","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Cleaned all brushes and brush holders with electro solve and cleaned the terminals and fixed it back.\t","2024-01-02T23:59:35","","Completed","2023-10-02T23:59:35","No","No","No","Internal"]
[null,null,null,32605,73214,"27_Sat Nov 18 2023 09:40:36 GMT+0800","2023-10-03T23:59:35","Defect","Ship Staff","Ship Staff Insp.","EGB water circulating pump found not operating from remote.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","","","","","same rectified and now pump can be operated from remote.","2024-01-03T23:59:35","","Completed","2023-10-03T23:59:35","No","No","No","Internal"]
[null,null,null,32555,15008,"0_Fri Oct 06 2023 08:17:40 GMT+0800","2023-10-05T23:59:35","Critical Equipment","Ship Staff","Ship Staff Insp.","Leak from wasted isolation valve of M2 mooring winch","Deck - Mooring Machinery","Mooring","Equipment Related","11.4","Very High","","","Spare valve received at Singapore in Jan 24. Same replaced and winch tried out found satisfactory.","2024-02-25T23:59:35","DLOT235068","Completed","2024-01-25T23:59:35","No","No","No","Internal"]
[null,null,null,32630,68229,"0_Sun Nov 19 2023 11:45:19 GMT+0800","2023-10-06T23:59:35","Defect","Ship Staff","Ship Staff Insp.","EGCS MGPS Cu anode found giving alarm found faulty PCB. opened the sea chest and checked the anode condition. ","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","cleaned the terminals checked the continuity found good. made connections to the spare  PCB in the panel itself and tried out. found satisfactory.","2024-01-05T23:59:35","","Completed","2023-10-06T23:59:35","No","No","No","Internal"]
[null,null,null,32581,37236,"27_Sun Oct 08 2023 09:23:30 GMT+0800","2023-10-07T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","VRCS Pump no. 1 found to be making abnormal noise during ballasting operations.  Same changeover to No.1 & completed the ballasting operations","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","Found pump not moving freely. New spare pump was replaced. ","2023-10-09T23:59:35","","Completed","2023-10-08T23:59:35","No","No","No","Internal"]
[null,null,null,32583,18680,"27_Sun Oct 08 2023 09:20:59 GMT+0800","2023-10-08T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Slop Port Dump Valve found to be leaking with tank IG","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","","","","","Dump valve surface cleaned and lubricated, leak rectified.","2023-11-07T23:59:35","","Completed","2023-11-01T23:59:35","No","No","No","Internal"]
[null,null,null,32606,15919,"27_Sat Nov 18 2023 09:43:53 GMT+0800","2023-10-09T23:59:35","Defect","Ship Staff","Ship Staff Insp.","7k-4k steam line safety valve found leaking and pressure gauge not working.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","",""," leak rectified and pressure gauge renewed.","2024-01-08T23:59:35","","Completed","2023-10-10T23:59:35","No","No","No","Internal"]
[null,null,null,32631,90240,"0_Sun Nov 19 2023 11:47:49 GMT+0800","2023-10-14T23:59:35","Defect","Ship Staff","Ship Staff Insp.","remote control panel in ECE of fwd and aft ICCP found showing incorrect readings.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","same rectified.","2024-01-12T23:59:35","","Completed","2023-10-14T23:59:35","No","No","No","Internal"]
[null,null,null,33325,21764,"27_Mon Dec 18 2023 11:28:10 GMT+0800","2023-10-17T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Cargo Audit","Vessel has 2 types of UTI's (open and restricted) calibration certificate available for open type while vessel is carrying high H2S cargo.","Miscellaneous","Cargo / Ballast Systems","Equipment Related","8.12","Medium","","","shore servicing / calibration carried out at Singapore","2024-01-16T23:59:35","DLOT230313 raised for shore servicing / calibration","Completed","2024-01-02T23:59:35","No","No","No","Internal"]
[null,null,null,32639,90571,"0_Sun Nov 19 2023 11:51:09 GMT+0800","2023-10-17T23:59:35","Defect","Ship Staff","Ship Staff Insp.","found few patches on EGB's body.\t\t\t\t\t\t\t\t\t\t\t\t\t\n","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","areas refitted with new metal sheet.\t\t\t","2024-01-16T23:59:35","","Completed","2023-10-17T23:59:35","No","No","No","Internal"]
[null,null,null,32607,70385,"27_Sat Nov 18 2023 09:46:52 GMT+0800","2023-10-18T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Aux boiler feed pump No.1 outlet valve found leaking.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","","","","","same renewed with the new valve and found no leaks.","2024-01-17T23:59:35","","Completed","2023-10-18T23:59:35","No","No","No","Internal"]
[null,null,null,32556,76501,"27_Sat Oct 21 2023 07:34:31 GMT+0800","2023-10-19T23:59:35","Non Conformity","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Sampling and Sndg tape on board not of restricted type","Miscellaneous","Cargo / Ballast Systems","Equipment Related","8.12","Medium","","","Spares received, same fitted , found satisfactory in operation.","2024-01-18T23:59:35","DLOT230283","Completed","2024-01-05T23:59:35","No","No","No","Internal"]
[null,null,null,32557,57761,"0_Sat Oct 21 2023 08:12:28 GMT+0800","2023-10-19T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Min level to be maintained in the stbd FW Tank to be marked (feed to hyper mist system)","Miscellaneous","Eng. / Strg. Comp.","Knowledge Based","","","","","Minimum quantity of 50 m3 to be kept in Fresh water tank stbd, same is stenciled on the tank bulkhead.","2024-01-31T23:59:35","","Completed","2024-01-12T23:59:35","No","No","No","Internal"]
[null,null,null,32558,64009,"0_Sat Oct 21 2023 08:17:20 GMT+0800","2023-10-19T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","GOODWOOD Standard Safety posters not available on board- Kindly liaise with Procure to arrange for a set of posters to be connected from Mumbai vendor to the vessel","Documentation","Cert. & Docu.","Inappropriate Procedure","","","","","Posters connected at Singapore, same posted at various locations.","2024-01-16T23:59:35","","Completed","2024-01-13T23:59:35","No","No","No","Internal"]
[null,null,null,32560,77437,"0_Sat Oct 21 2023 08:46:56 GMT+0800","2023-10-19T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Isolation valves (fire and foam line) not holding – same to be overhauled","Deck - Pipe / Fittings","Safety / LSA / FFA","Equipment Related","5.38","High","","","Suspected valve was opened up for inspection, seatring and disc found to be intact, surfaces cleaned and valve boxed back.","2024-01-16T23:59:35","","Completed","2023-12-14T23:59:35","No","No","No","Internal"]
[null,null,null,32561,78625,"0_Sat Oct 21 2023 07:40:41 GMT+0800","2023-10-19T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Light fittings around accommodation are corroded, surface preparation to be carried out and if required sections to be renewed","Accommodation","General Appearance","External Factors","11.11","Very High","","","Wasted section for light fittings support is replaced with fabricated spare.","2024-01-23T23:59:35","","Completed","2024-01-15T23:59:35","No","No","No","Internal"]
[null,null,null,32562,82934,"0_Sat Oct 21 2023 08:18:45 GMT+0800","2023-10-19T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Hot water in the accommodation is reddish in color","Accommodation","MLC Related","Equipment Related","","","","","Calorifier have been cleaned twice, issue is under observation now.","2024-01-02T23:59:35","","Completed","2024-01-02T23:59:35","No","No","No","Internal"]
[null,null,null,32563,57517,"0_Sat Oct 21 2023 07:43:30 GMT+0800","2023-10-19T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Deck seal drain and overboard line sections to be renewed","Deck - Pipe / Fittings","General Appearance","External Factors","11.4","Very High","","","Line sections renewed as required.","2024-01-16T23:59:35","","Completed","2023-12-02T23:59:35","No","No","No","Internal"]
[null,null,null,32564,84885,"0_Sat Oct 21 2023 08:49:42 GMT+0800","2023-10-19T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Work shop flame retardant curtain not approved type , sufficient length and height for the area and holed","Miscellaneous","Eng. / Strg. Comp.","Knowledge Based","5.25","Medium","","","Requisition received onboard at Singapore in Jan 24. Spare flame retardant curtain replaced with new spare.","2024-01-23T23:59:35","DLOT230270 ","Completed","2024-01-22T23:59:35","No","No","No","Internal"]
[null,null,null,32565,91587,"0_Sat Oct 21 2023 08:51:16 GMT+0800","2023-10-19T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Chain block CB12 safety latch damaged","Miscellaneous","Eng. / Strg. Comp.","Human Error","8.50","Medium","","","Safety latch repaired","2024-01-16T23:59:35","","Completed","2023-11-20T23:59:35","No","No","No","Internal"]
[null,null,null,32566,54443,"0_Sat Oct 21 2023 08:52:14 GMT+0800","2023-10-19T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","SCBA bottles have a300 bar px rating, while EEBD have 200 bar px rating, same BA compressor with relief valve at 330 bar used for filling EEBD, appropriate relive valve for EEBD Filling","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","Spare relief valve received for the same at Singapore in Jan 24. Tried out the operation found satisfactory.","2024-01-20T23:59:35","DLOT230276","Completed","2024-01-22T23:59:35","No","No","No","Internal"]
[null,null,null,32567,16834,"27_Sat Oct 21 2023 08:37:54 GMT+0800","2023-10-19T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Side lights – Background not matte finish and installation not in line with requirements (sector slightly off by 5 to 8 degrees) due to loose door hinge","Miscellaneous","ISM Related","Equipment Related","","","","","Side light background painted matt black and loose door hinge secured properly","2024-01-16T23:59:35","","Completed","2023-11-30T23:59:35","No","No","No","Internal"]
[null,null,null,32568,34760,"0_Sat Oct 21 2023 07:42:23 GMT+0800","2023-10-19T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Crack noted on pipe line support for Fire line (outside Port side pumproom entrance)","Deck - Pipe / Fittings","General Appearance","External Factors","11.5","Medium","","","New support is fabricated and fitted/welded in place, found satisfactory.","2024-01-22T23:59:35","","Completed","2024-01-16T23:59:35","No","No","No","Internal"]
[null,null,null,32569,87140,"0_Sat Oct 21 2023 08:53:32 GMT+0800","2023-10-19T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Tongue type bow stopper for ETA/ SPM ‘s locking pin has play larger than permitted. Vessel to prepare sleeve to reduce gap to permissible range","Miscellaneous","Mooring","Equipment Related","","","","","New sleeves fabricated and fitted in place.","2024-01-22T23:59:35","","Completed","2024-01-15T23:59:35","No","No","No","Internal"]
[null,null,null,32579,20784,"0_Mon Nov 20 2023 05:42:37 GMT+0800","2023-10-19T23:59:35","Defect","Ship Staff","Ship Staff Insp.","#2 HFO service tank steam heating bypass valve leaking from valve body - Globe valve","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Vessel received spares for the same at Singapore in Jan 24. Valve replaced with new spare. Found satisfactory without any leakages.\n\n","2024-04-30T23:59:35","DLOT230274 ","Completed","2024-02-10T23:59:35","No","No","No","Internal"]
[null,null,null,32582,73282,"0_Sat Oct 21 2023 08:54:23 GMT+0800","2023-10-19T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","SEEEMP Posters/ labels not posted","Documentation","ISM Related","Behaviour Based","","","","","Posters posted at required places","2024-01-16T23:59:35","","Completed","2023-10-27T23:59:35","No","No","No","Internal"]
[null,null,null,32584,58223,"0_Sat Oct 21 2023 08:09:29 GMT+0800","2023-10-19T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Galley drains chocked","Accommodation","MLC Related","Industry Issue","11.13","Low","","","Galley drains cleared throughly","2024-01-16T23:59:35","","Completed","2023-11-13T23:59:35","No","No","No","Internal"]
[null,null,null,32585,93230,"0_Sat Oct 21 2023 08:47:51 GMT+0800","2023-10-19T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","I beam above no 3 Aux eng not marked with SWL","E/R - Aux. Engine","Eng. / Strg. Comp.","Human Error","","","","","stencilling to be done","2024-01-16T23:59:35","","Completed","2023-10-19T23:59:35","No","No","No","Internal"]
[null,null,null,32586,72107,"0_Sat Oct 21 2023 08:16:01 GMT+0800","2023-10-19T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Bottom gauge push button for gauge glass of Feed water tank noted compressed and not closing when released.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.25","Very High","","","Gauge push button  freed up, working satisfactory.","2024-01-16T23:59:35","","Completed","2023-10-19T23:59:35","No","No","No","Internal"]
[null,null,null,32624,58162,"0_Sat Oct 21 2023 08:14:05 GMT+0800","2023-10-19T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Leak noted at Boiler feed water valve","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Leak  rectified","2024-01-16T23:59:35","","Completed","2023-10-20T23:59:35","No","No","No","Internal"]
[null,null,null,32625,71200,"0_Sat Oct 21 2023 08:11:29 GMT+0800","2023-10-19T23:59:35","Non Conformity","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Drain channels of steering gear blocked by 200 ltr drums","Miscellaneous","Eng. / Strg. Comp.","Human Error","10.42","Medium","","","Drain channels  cleared by shifting 200 ltrs drums","2024-01-16T23:59:35","","Completed","2023-10-25T23:59:35","No","No","No","Internal"]
[null,null,null,32609,85893,"27_Sat Nov 18 2023 09:49:17 GMT+0800","2023-10-20T23:59:35","Defect","Ship Staff","Ship Staff Insp.","EGCS WMS-1 de-bubbler was found leaking.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","","","","","same rectified by changing O-ring in plexi glass and fixed back. found no leaks.","2024-01-19T23:59:35","","Completed","2023-10-20T23:59:35","No","No","No","Internal"]
[null,null,null,32610,65075,"27_Sat Nov 18 2023 09:52:18 GMT+0800","2023-10-21T23:59:35","Defect","Ship Staff","Ship Staff Insp.","FWD ICCP cooling fan in the heat sink was found not working.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","changed the fan with spare and switched ICCP to auto. found working satisfactory.",null,"","Completed","2023-10-21T23:59:35","No","No","No","Internal"]
[null,null,null,32611,57210,"27_Sat Nov 18 2023 09:55:30 GMT+0800","2023-10-23T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Flywheel intermediate shaft reamed nut found loose and out of place.\t\t\t\n","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","same fitted with the new spare nut. ","2024-01-23T23:59:35","","Completed","2023-10-23T23:59:35","No","No","No","Internal"]
[null,null,null,32614,12731,"27_Sat Nov 18 2023 10:07:16 GMT+0800","2023-10-24T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Emergency fire pump discharge valve found leaking. ","E/R - Pipes/ valves & fittings,E/R - Pumps","Emgcy. Systems","Equipment Related","","","","","valve seat inspected and lapping work carried out and put back in place found satisfactory.","2024-01-24T23:59:35","","Completed","2023-10-24T23:59:35","No","No","No","Internal"]
[null,null,null,32612,63101,"27_Sat Nov 18 2023 09:59:26 GMT+0800","2023-10-25T23:59:35","Defect","Ship Staff","Ship Staff Insp.","IG Blower #1 and #2 drain line found leaking.\t\t\t\t\t\t\t\t\t\t\t\t\t\n","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","same rectified by welding in ER workshop.","2024-01-25T23:59:35","","Completed","2023-10-25T23:59:35","No","No","No","Internal"]
[null,null,null,32620,65246,"27_Sat Nov 18 2023 10:03:25 GMT+0800","2023-10-26T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Vacuum condensers one anode found damaged.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","same renewed and cleaning carried out. Rubber coatings inspected and found to be satisfactory.","2024-01-26T23:59:35","","Completed","2023-10-26T23:59:35","No","No","No","Internal"]
[null,null,null,32615,83579,"27_Sat Nov 18 2023 10:09:45 GMT+0800","2023-10-28T23:59:35","Defect","Ship Staff","Ship Staff Insp.","LT cooler #2 SW outlet pipe reducer's body found leaking.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","same renewed with new fabricated piece. found satisfactory.","2024-01-27T23:59:35","","Completed","2023-10-28T23:59:35","No","No","No","Internal"]
[null,null,null,32622,64429,"27_Sat Nov 18 2023 10:17:21 GMT+0800","2023-10-29T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Horn control unit reported not working after lightening .Checked and found mains fuse outside as well as inside blown off.\t\t\t\t\t\t","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","Unit dismantled and renewed fuses. Found Power Led is ON when we press Power Button. But no other key are responding (no output as well as no LED Indication). As of now Fwd whistle made operational through push buttons in wheel house.\t\t\t\t\t\t\t","2024-01-27T23:59:35","","Completed","2023-10-29T23:59:35","No","No","No","Internal"]
[null,null,null,32616,94149,"27_Sat Nov 18 2023 10:12:46 GMT+0800","2023-10-31T23:59:35","Defect","Ship Staff","Ship Staff Insp.","LT cooler #2  SW inlet pipe found leaking due to pin hole on the weld seam of the pipe.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Hot work carried out in E/R workshop on the weld seam and pipe put back in place. found satisfactory.","2024-01-30T23:59:35","","Completed","2023-10-31T23:59:35","No","No","No","Internal"]
[null,null,null,32621,46340,"27_Sat Nov 18 2023 10:36:01 GMT+0800","2023-11-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","LT cooler #1 SW outlet and  backwash inlet valves found leaking at the pipe flanges.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","valves renewed and LT cooler #1 SW outlet pipe leak at the pipe flange repaired by hot work in E/R workshop.","2024-01-31T23:59:35","","Completed","2023-11-01T23:59:35","No","No","No","Internal"]
[null,null,null,32633,93083,"0_Sun Nov 19 2023 11:57:42 GMT+0800","2023-11-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","slip ring found faulty.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","Slip ring dismantled and cleaned both slip ring and shaft fitted back and checked Continuity BW slip ring and shaft is 0 ohms. Current measured BW slip ring and shaft at 2 places (180 deg apart). 4.58 A and 4.6 A .Short circuit current of Battery ( D cell)used 4.7 A","2024-02-01T23:59:35","","Completed","2023-11-01T23:59:35","No","No","No","Internal"]
[null,null,null,32617,21078,"27_Sat Nov 18 2023 10:15:02 GMT+0800","2023-11-02T23:59:35","Defect","Ship Staff","Ship Staff Insp.","S/G room bilge well float sensor found  broken.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","same renewed with the new spare.\t","2024-02-01T23:59:35","","Completed","2023-11-02T23:59:35","No","No","No","Internal"]
[null,null,null,32619,50631,"27_Sat Nov 18 2023 10:33:33 GMT+0800","2023-11-02T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Air ejector sea water inlet and outlet valve found leaking.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","valves renewed with the new spare. found no leaks.","2024-02-01T23:59:35","","Completed","2023-11-02T23:59:35","No","No","No","Internal"]
[null,null,null,32623,96215,"0_Sat Nov 18 2023 10:37:48 GMT+0800","2023-11-02T23:59:35","Defect","Ship Staff","Ship Staff Insp.","LT cooler #2 SW backwash outlet valve found leaking and SW outlet pipe having a hole near the pipe flange.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","valve renewed and SW outlet pipe having a hole near the pipe flange repaired by hot work in E/R workshop.","2024-02-01T23:59:35","","Completed","2023-11-02T23:59:35","No","No","No","Internal"]
[null,null,null,32577,93300,"0_Mon Nov 20 2023 05:39:11 GMT+0800","2023-11-03T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Grey water valve to Sewage is damaged - DN65 gate valve. ","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","",""," Grey water valve to Sewage is damaged - DN65 gate valve needs renewal. Spares received for the same at Singapore in Jan 24. Spare valve replaced with the defective one, now found satisfactory.","2024-02-03T23:59:35","DLOT230274","Completed","2024-01-22T23:59:35","No","No","No","Internal"]
[null,null,null,32634,20002,"0_Sun Nov 19 2023 11:58:58 GMT+0800","2023-11-03T23:59:35","Defect","Ship Staff","Ship Staff Insp.","EGB inlet damper was not operating from ECR. Same checked and found control air pipe was leaking. ","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","Same rectified and now it is working satisfactory.","2024-02-03T23:59:35","","Completed","2023-11-03T23:59:35","No","No","No","Internal"]
[null,null,null,32635,28387,"0_Sun Nov 19 2023 12:00:25 GMT+0800","2023-11-04T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Reported that VSAT phone is not responding \t\t\t\t\t\t\t\t\t\t\t\t\t","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","same checked and swap the terminals in switch with CCR and tried out both phones both working satisfactory.\t\t\t\t\t","2024-02-03T23:59:35","","Completed","2023-11-04T23:59:35","No","No","No","Internal"]
[null,null,null,32637,57872,"0_Sun Nov 19 2023 12:03:43 GMT+0800","2023-11-05T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Bottom platform hanging light pendent found giving 220v low insulation from cable.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","same renewed with new cable.","2024-02-05T23:59:35","","Completed","2023-11-05T23:59:35","No","No","No","Internal"]
[null,null,null,32638,84012,"0_Sun Nov 19 2023 12:05:33 GMT+0800","2023-11-06T23:59:35","Defect","Ship Staff","Ship Staff Insp.","STBD wing RPM indicator was malfunctioning, \t\t\t\t\t\t\t\t","Navigation - Others","Navigation","Equipment Related","","","","","same renewed with new RPM indicator.\t\t\t\t\t\t\t\t\t\t","2024-02-05T23:59:35","","Completed","2023-11-06T23:59:35","No","No","No","Internal"]
[null,null,null,32618,26373,"27_Sat Nov 18 2023 10:31:05 GMT+0800","2023-11-07T23:59:35","Defect","Ship Staff","Ship Staff Insp.","FWG ejector pump found tripped while in operation, upon inspection found the rotor touching the stator at a particular position.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","","","","","Motor dismantled & found the driving end bearing damaged, after removal of the bearing noticed the bearing seat completely damaged. The motor replaced with spare and made operational. working satisfactory.","2024-02-06T23:59:35","","Completed","2023-11-07T23:59:35","No","No","No","Internal"]
[null,null,null,32641,58402,"0_Sun Nov 19 2023 12:07:20 GMT+0800","2023-11-08T23:59:35","Defect","Ship Staff","Ship Staff Insp.","AE3 viscotherm found showing error in control panel. \t\t\t\t\t\t\t\t\t\t\n","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Same opened, cleaned and boxed back. working satisfactory.\t\t\t\t\t\t\t\t","2024-02-11T23:59:35","","Completed","2023-11-11T23:59:35","No","No","No","Internal"]
[null,null,null,32642,85356,"0_Sun Nov 19 2023 12:09:30 GMT+0800","2023-11-11T23:59:35","Defect","Ship Staff","Ship Staff Insp.","WBP NO.2 mechanical seal found leaking.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","","","","","same renewed with the new spare and pump tried out, found satisfactory.\n","2024-02-11T23:59:35","","Completed","2023-11-11T23:59:35","No","No","No","Internal"]
[null,null,null,32643,48464,"0_Sun Nov 19 2023 12:11:39 GMT+0800","2023-11-14T23:59:35","Defect","Ship Staff","Ship Staff Insp.","AE #3, unit 5 exhaust valve found damaged.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","cylinder head and exhaust valve renewed.","2024-02-14T23:59:35","","Completed","2023-11-14T23:59:35","No","No","No","Internal"]
[null,null,null,32570,21881,"27_Sun Nov 19 2023 07:21:56 GMT+0800","2023-11-15T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Exhaust leaking from ME # 1 T/C outlet bellow","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","",""," ME # 1 T/C outlet bellow inspected, found bellow cracked. Temporary repairs caried out by cold work. Lagging as completely damaged, same renewed. Some bolts found loose, same were retightened. New bellow is on order, need to be replaced once received.\nNew bellow received in Singapore, same replaced by shore team at Singapore jan 24. New bellow with new lagging and gaskets replaced. The bellow is fabricated by shore workshop.","2024-02-15T23:59:35","","Completed","2024-01-03T23:59:35","No","No","No","Internal"]
[null,null,null,32571,22381,"0_Sun Nov 19 2023 07:24:13 GMT+0800","2023-11-15T23:59:35","Defect","Ship Staff","Ship Staff Insp.","EGB bypass damper outlet bellow leaking","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","EGB bypass damper outlet bellow inspected, fund bellow & gasket intact. However the lagging was completely damaged, same renewed. Bolts found loose, same were retightened.","2024-02-15T23:59:35","","Completed","2023-12-17T23:59:35","No","No","No","Internal"]
[null,null,null,32576,90395,"0_Sun Nov 19 2023 07:28:14 GMT+0800","2023-11-15T23:59:35","Defect","Ship Staff","Ship Staff Insp.","# 1 & # 2 accommodation AHU fresh air intake dampers wasted & beyond repair","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","# 1 &  # 2 accommodation AHU fresh air intake dampers repaired by fabricating new flaps.","2024-02-15T23:59:35","","Completed","2023-12-06T23:59:35","No","No","No","Internal"]
[null,null,null,32644,27578,"27_Sun Nov 19 2023 12:15:37 GMT+0800","2023-11-15T23:59:35","Defect","Ship Staff","Ship Staff Insp.","AE #1 pick-up sensor found faulty.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","sensor renewed and DG made operational.","2024-02-14T23:59:35","","Completed","2023-11-15T23:59:35","No","No","No","Internal"]
[null,null,null,32984,65263,"27_Thu Nov 30 2023 08:07:07 GMT+0800","2023-11-22T23:59:35","Defect","Ship Staff","Ship Staff Insp.","# 1 Boiler water circulating pump tripped on overload while in operation. \nUpon inspection, found that the pump is not rotating as the bearings were seized & also the pump found leaking excessively from the mechanical seal.\n\n\n","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","","","","","# 1 Boiler water circulating pump overhauled with new mechanical seal & fitted back, tried out. Found working satisfactory.","2024-02-20T23:59:35","","Completed","2023-11-22T23:59:35","No","No","No","Internal"]
[null,null,null,32985,20767,"27_Thu Nov 30 2023 08:09:24 GMT+0800","2023-11-23T23:59:35","Defect","Ship Staff","Ship Staff Insp.","LO purifier no.2 drive belt found damaged. ","E/R - Purifier","Eng. / Strg. Comp.","Equipment Related","","","","","Drive belt replaced with new spare.","2024-02-23T23:59:35","","Completed","2023-11-23T23:59:35","No","No","No","Internal"]
[null,null,null,32980,61920,"0_Thu Nov 30 2023 08:20:59 GMT+0800","2023-11-24T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Aux eng No.3 FCU fuel oil auto backwash filter actuator found not working. ","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","PLC for actuator control found malfunctioning, RO - DLOT230286 raised. Spares received in Singapore Jan 24, same replaced, Auto backwash filter operation tried out, found satisfactory.","2024-02-24T23:59:35","RO - DLOT230286 raised.","Completed","2024-01-10T23:59:35","No","No","No","Internal"]
[null,null,null,32976,84975,"27_Sun Dec 03 2023 08:33:01 GMT+0800","2023-11-25T23:59:35","Defect","Ship Staff","Ship Staff Insp.","# 1 Accommodation A/C compressor discharge shut of valve not holding.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Needs replacement, RO - DLOT230302 raised., Spares received in Singapore Jan 24, shore technician replaced discharge valve. ","2024-02-25T23:59:35","RO - DLOT230302 raised.","Completed","2024-01-03T23:59:35","No","No","No","Internal"]
[null,null,null,32986,69013,"0_Thu Nov 30 2023 08:26:45 GMT+0800","2023-11-25T23:59:35","Defect","Ship Staff","Ship Staff Insp.","DG#3 LO priming pump motor found making noise.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","DG#3 LO priming pump motor overhauled, found working satisfactory.","2024-02-29T23:59:35","","Completed","2023-11-25T23:59:35","No","No","No","Internal"]
[null,null,null,32989,66741,"0_Thu Nov 30 2023 08:30:26 GMT+0800","2023-11-26T23:59:35","Defect","Ship Staff","Ship Staff Insp.","PA and talk back system which reported as not working.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","Checked the same and found four speakers in accommodation are not working, All four speakers replaced with new spare.\t\t\t\t\t\t\t\t\t\t\t\t\t\t\t\t\t\t\n","2024-02-26T23:59:35","","Completed","2023-11-26T23:59:35","No","No","No","Internal"]
[null,null,null,32982,30121,"27_Sun Dec 03 2023 12:25:09 GMT+0800","2023-11-27T23:59:35","Defect","Ship Staff","Ship Staff Insp.","BWTS #1 rectifier triggering overcurrent fault.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","",""," The defective CT for # 1 rectifier unit replaced with new spare & the BWTS system made opeartional.","2024-02-27T23:59:35","","Completed","2023-12-09T23:59:35","No","No","No","Internal"]
[null,null,null,32983,11361,"0_Sun Dec 03 2023 08:35:07 GMT+0800","2023-11-28T23:59:35","Defect","Ship Staff","Ship Staff Insp.","ME LO cooler temperature controller not working","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Pilot relay opened up, inspected diaphragm. All found satisfactory. The controller is put in use, will close DDRL once operation is found satisfactory while maneuvering. Operation found satisfactory during maneuvering.","2024-03-30T23:59:35","","Completed","2024-02-12T23:59:35","No","No","No","Internal"]
[null,null,null,33328,10494,"0_Mon Dec 18 2023 17:04:30 GMT+0800","2023-11-29T23:59:35","Defect","Ship Staff","Ship Staff Insp.","ME unit 4. Exh. Gas temp sensor found malfunctioning. ","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","Renewed Exh. Gas temp sensor for ME unit 4.","2024-02-29T23:59:35","","Completed","2023-11-29T23:59:35","No","No","No","Internal"]
[null,null,null,33331,31932,"0_Mon Dec 18 2023 17:02:06 GMT+0800","2023-11-29T23:59:35","Defect","Ship Staff","Ship Staff Insp.","ME Lube oil auto backwash filter STBD side chamber hydraulic motor found malfunctioning.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","ME Lube oil auto backwash filter STBD side chamber hydraulic motor overhauled. & made operational.","2024-02-29T23:59:35","","Completed","2023-11-30T23:59:35","No","No","No","Internal"]
[null,null,null,32987,33466,"27_Sat Dec 02 2023 14:10:17 GMT+0800","2023-11-29T23:59:35","Defect","Ship Staff","Ship Staff Insp.","ME auto backwash filter hydraulic motor found malfunctioning.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","ME auto backwash filter hydraulic motor bearings & O-rings renewed, made operational.","2024-02-29T23:59:35","","Completed","2023-11-29T23:59:35","No","No","No","Internal"]
[null,null,null,32979,90347,"27_Sat Dec 02 2023 14:12:53 GMT+0800","2023-11-30T23:59:35","Defect","Ship Staff","Ship Staff Insp.","# 2 Aux Boiler Local control panel display not working.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","RO - DLOT235083 received in Singapore jan 24, Aux boiler local control panel display replaced with new spare.","2024-03-01T23:59:35","","Completed","2024-01-09T23:59:35","No","No","No","Internal"]
[null,null,null,32988,99065,"27_Sat Dec 02 2023 14:15:00 GMT+0800","2023-12-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","ME # 4 unit Exhaust gas temperature sensor found malfunctioning.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","ME # 4 unit Exhaust gas temperature sensor replaced with new spare.","2024-03-01T23:59:35","","Completed",null,"No","No","No","Internal"]
[null,null,null,33330,82917,"0_Mon Dec 18 2023 16:56:29 GMT+0800","2023-12-10T23:59:35","Defect","Ship Staff","Ship Staff Insp.","#1 Atmospheric condenser SW inlet pipe found leaking. ","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Leaky pipe section removed from place, hot work and painting carried out in E/R workshop and Anodes renewed.  Same put back and condenser tried out. Found satisfactory.","2024-03-10T23:59:35","","Completed","2023-12-10T23:59:35","No","No","No","Internal"]
[null,null,null,33329,99944,"0_Mon Dec 18 2023 16:58:47 GMT+0800","2023-12-16T23:59:35","Defect","Ship Staff","Ship Staff Insp.","No.2 Aux boiler atomising air-steam actuator found malfunctioning.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","No.2 Aux boiler atomising air-steam actuator renewed with new spare.","2024-03-16T23:59:35","","Completed","2023-12-16T23:59:35","No","No","No","Internal"]
[null,null,null,33804,63306,"27_Tue Jan 30 2024 02:12:45 GMT+0800","2024-01-02T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Port windlass bow stopper securing pin bended","Deck - Mooring Machinery","Mooring","Equipment Related","10.3","Medium","","","The securing pin was straightened","2024-02-01T23:59:35","N/A","Completed","2024-01-29T23:59:35","No","No","No","Internal"]
[null,null,null,33796,98524,"27_Sat Jan 27 2024 22:03:53 GMT+0800","2024-01-03T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Steam inlet root valve to Main engine fuel oil heaters is leaking, same to be rectified.","","Eng. / Strg. Comp.","Equipment Related","","","","","Steam inlet valve to be replaced with new spare. Vessel is at sea, same can be done while in port or when change over to LSMGO. Inlet valve overhauled, topped up with new gland packing, fitted back in place, no leak observed.","2024-03-30T23:59:35","","Completed","2024-02-12T23:59:35","No","No","No","Internal"]
[null,null,null,33799,53449,"27_Sat Jan 27 2024 22:10:47 GMT+0800","2024-01-03T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","IG scrubber inert gas inlet pipe is having flexible hose for washing/cooling inert gas, same is leaking, become brittle with age.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Flexible pipes to be replaced with new spares. Flexible rubber hose replaced with new spare.","2024-03-30T23:59:35","","Completed","2024-02-21T23:59:35","No","No","No","Internal"]
[null,null,null,33802,87789,"27_Sat Jan 27 2024 18:51:13 GMT+0800","2024-01-03T23:59:35","Breakdown","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Fresh water hypermist system pump distribution tower is having leaks from various plastic pipe fittings.","","Eng. / Strg. Comp.","Equipment Related","","","","","The distribution tower overhauled, various other pipe section found to be cracked and brittle, all pipe sections replaced with brass pipes, found there is no leak.","2024-02-03T23:59:35","","Completed","2024-01-23T23:59:35","No","No","No","Internal"]
[null,null,null,33803,46918,"27_Sat Jan 27 2024 22:17:06 GMT+0800","2024-01-03T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Aux engine no.3 Auto backwash filter drain valve flange gasket is found to be leaking.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Drain valve gasket is replaced, tried out auto back wash filter found no leak from drain valve.","2024-02-03T23:59:35","","Completed","2024-01-10T23:59:35","No","No","No","Internal"]
[null,null,null,33789,21628,"27_Sat Jan 27 2024 21:58:36 GMT+0800","2024-01-03T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Engine control room is found to be untidy with manuals scattered and not arranged","Documentation","Eng. / Strg. Comp.","Behaviour Based","","","","","All the file documents, manuals cabinets is properly arranged and engine control room to be kept in tidy condition. Various electrical socket connection for computer and printer are secured and arranged.","2024-03-30T23:59:35","","Completed","2024-02-10T23:59:35","No","No","No","Internal"]
[null,null,null,33790,14569,"27_Sat Jan 27 2024 22:14:44 GMT+0800","2024-01-03T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Aft mooring winch hydraulic tank gauge glass is leaking.","Deck - Machinery,Deck - Mooring Machinery","Eng. / Strg. Comp.","Equipment Related","","","","","Aft mooring winch hydraulic tank to be emptied, gauge glass packing to be replaced with new spare/fabricated. The gauge glass is tightened and leak is arrested. ","2024-04-30T23:59:35","","Completed","2024-02-10T23:59:35","No","No","No","Internal"]
[null,null,null,33801,54747,"27_Fri Jan 12 2024 18:33:31 GMT+0800","2024-01-11T23:59:35","Breakdown,Defect","Ship Staff","Ship Staff Insp.","Port provision crane is having hydraulic oil leak through fittings, other fittings are also rusted.","Deck - Machinery","Cargo / Ballast Systems","Equipment Related","","","","","Defective Hydraulic oil line fitting to be identified and replaced with new spare. Various other fittings to be made rust free and covered with denzo tape. Defective hydraulic fittings replaced with new fittings.","2024-02-19T23:59:35","","Completed","2024-01-19T23:59:35","No","No","No","Internal"]
[null,null,null,33800,37952,"27_Fri Feb 02 2024 19:41:29 GMT+0800","2024-01-31T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Soot tank outlet line to the outlet valve is holed and repaired with cordobond.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","New pipe section to be fabricated and replaced. New pipe section fitted in place, soot tank cleaned and freshly painted with epoxy paint.","2024-04-30T23:59:35","","Completed","2024-02-28T23:59:35","No","No","No","Internal"]
[null,null,null,null,73506,"27_Fri Mar 15 2024 16:21:13 GMT+0800","2024-03-01T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Daily bilge pump is leaking from gland packing.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","","","","","Daily bilge pump gland packing to renewed. The gland is tightened, pump is under observation for further leaks.","2024-04-30T08:00:00","","Completed","2024-04-06T08:00:00","No","No","No","Internal"]
[null,null,null,null,43174,"27_Fri Mar 15 2024 16:05:30 GMT+0800","2024-03-01T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Engine room vent fans suction mesh frame is broken at sections.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Engine room vent fans suction mesh frame is broken at few section, same to be removed and fabricate with new frame for the suction mesh on top of vent fan. Vent fan suction mesh frame secured firmly, cleaned thoroughly and fitted back.","2024-04-30T08:00:00","","Completed","2024-03-30T08:00:00","No","No","No","Internal"]
[null,null,null,null,63722,"27_Fri Mar 15 2024 01:19:39 GMT+0800","2024-03-01T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Fixed gas detector for ballast tank with FLOW FAIL alarm when connected on line.","Hull & Tanks","Cargo / Ballast Systems","Equipment Related","5.21","Medium","","","Under investigation. The fixed gas detection system solenoid valves overhauled, sampling pump overhauled, all parts cleaned and fitted back. System is operational.","2024-04-30T08:00:00","","Completed","2024-03-30T08:00:00","No","No","No","Internal"]
[null,null,null,null,58085,"27_Fri Mar 15 2024 00:08:02 GMT+0800","2024-03-01T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Draft gauges readings in the CCR defective.","Hull & Tanks","Cargo / Ballast Systems","Equipment Related","8.8","Medium","","","Technician attended at last call Singapore on 02 Jan 2024. As per their assessment these sensors require renewal.\nShip's staff installed new sensor for Fwd and Port midship and with\nattended Technician at Singapore on 22-Apr-24 serviced and rectified the same.","2024-05-11T08:00:00","","Completed","2024-04-22T08:00:00","No","No","No","Internal"]
[null,null,null,null,87912,"27_Fri Mar 15 2024 00:12:31 GMT+0800","2024-03-01T08:00:00","Observation","Ship Staff","Ship Staff Insp.","Mooring tails renewal due on 06-May-24. ","","Mooring","Equipment Related","9.5","High","","","PO DLOT240038 raised - awaiting supply.\n21-Apr-24 Total 20 pcs of Mooring tails rcvd at Singapore and replaced the old tails on board.","2024-04-30T08:00:00","PO DLOT240038 raised.","Completed","2024-04-21T08:00:00","No","No","No","Internal"]
[null,null,null,null,46667,"27_Thu Mar 14 2024 23:33:02 GMT+0800","2024-03-01T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Deck seal steam line wastage.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.36","Medium","","","1. Dismantled and planned for renewal.\n2. Onboard fabrication completed, installed and painted.","2024-04-30T08:00:00","","Completed","2024-04-02T08:00:00","No","No","No","Internal"]
[null,null,null,null,65670,"27_Thu Mar 14 2024 18:18:12 GMT+0800","2024-03-01T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Ballast eductor valve BEV64 defective. Disc and shaft bended with crack on the disc. ","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.11","Medium","","","PO DLOT245022  raised. Temporary valve dismantled and in the ER workshop to straighten same.\nRcvd new valve at Singapore on 21-Apr-24, installed and tested satisfactory.","2024-04-30T08:00:00","PO DLOT245022 ","Completed","2024-04-29T08:00:00","No","No","No","Internal"]
[null,null,null,null,44969,"27_Sat Jan 27 2024 22:12:44 GMT+0800","2024-01-02T08:00:00","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","PV breaker gauge glass and spring loaded valve defective","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","9.16","High","","","1. PO raised and awaiting supply. Target date is revised. The gauge glass colour has become shady and dark  , making the level to be difficult to be visible. The gauge glass is intact in its operation.\n2. Glass gauge rcvd at Singapore on 3-Apr-24 and installed.","2024-04-30T08:00:00","DLOT240011 -PV BREAKER GAUGE GLASS\n","Completed","2024-04-04T08:00:00","No","No","No","Internal"]
[null,null,null,null,93363,"27_Wed Mar 29 2023 23:55:41 GMT+0800","2024-01-01T08:00:00","Other","Ship Staff","Ship Staff Insp.","Fwd & Port midhsip Draft values not displaying in CCR","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.8","Medium","","","1. Service technician attended in Singapore. Fwd & midship port sensor require to replace.\n2. Fwd and Port midship sensors replaced,  Technician attended in Singapore on 22-Apr-24 and rectify the same.","2024-04-01T08:00:00","","Completed","2024-04-22T08:00:00","No","No","No","Internal"]
[null,null,null,null,80275,"27_Fri Nov 24 2023 03:26:10 GMT+0800","2023-11-24T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Ballast eductor remote hydraulic valve (BEV 64- Ballast Eductor Valve) not opening completely upon operation. Upon inspection of valve found that the valve disc has a crack & deformation. Also, the shaft is bent. ","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","","","","","1. Valve required to renew, DLOT230281 raised.\n2. New valve rcvd at Singapore on 21-Apr-24, installed and tried out satisfactory.","2024-04-30T08:00:00"," DLOT230281","Completed","2024-04-29T08:00:00","No","No","No","Internal"]
[null,null,null,null,35728,"27_Fri Dec 01 2023 09:38:51 GMT+0800","2023-11-30T08:00:00","Observation","Ship Staff","Ship Staff Insp.","Bridge wing rudder angle indicator is erratic","Navigation - Others","Navigation","Equipment Related","4.7","High","","","Requisition raised for the same.\nSpare received and renewed","2024-04-30T08:00:00","DLOT240003","Completed","2024-04-29T08:00:00","No","No","No","Internal"]
[null,null,null,null,70214,"27_Fri Mar 15 2024 00:47:48 GMT+0800","2024-03-01T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Loadicator not on line after installation of the new fitted hard drive . System working in offline mode only","Deck - Mooring Machinery","Cargo / Ballast Systems","Equipment Related","9.7","Medium","","","As per office , online system is not mandatory and hence no further action required","2024-04-30T08:00:00","","Completed","2024-04-22T08:00:00","No","No","No","Internal"]
[null,null,null,null,92895,"27_Fri Mar 15 2024 16:46:37 GMT+0800","2024-03-01T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Main cooling sea water pump common discharge valve is frozen stuck in partial open condition.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Main cooling sea water pump common discharge valve is stuck frozen in open condition, same to be replaced with spare new valve. LT coolers to be isolated to carry out this job. Valve replaced with new spare, at Singapore April 23.","2024-04-30T08:00:00","","Completed","2024-04-23T08:00:00","No","No","No","Internal"]
[null,null,null,null,77281,"27_Fri Mar 15 2024 16:28:08 GMT+0800","2024-03-01T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Main cooling sea water pump suction valve is having a temporary repair to arrest sea water leak.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","The suction valve in the common line for Main cooling sea water pump no.2 is having a temporary repair work. The old valve to be replaced with new valve. Valve replaced with new spare at Singapore April 24","2024-04-30T08:00:00","","Completed","2024-04-23T08:00:00","No","No","No","Internal"]
[null,null,null,null,30481,"27_Fri Mar 15 2024 00:20:48 GMT+0800","2024-03-01T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Hot water calorfier is leaking of fresh water from the casing underneath the insulation.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Hot water calorifier need to be isolated, man hole cover to be opened up to identify the leakage. Leakage rectified.","2024-04-30T08:00:00","","Completed","2024-05-09T08:00:00","No","No","No","Internal"]
[null,null,null,null,92629,"27_Thu Mar 14 2024 23:37:02 GMT+0800","2024-03-01T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Sea water overboard line for LT coolers pipe section elbow is leaking above sea chest valve stbd side. The pipe is having a hole.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","We need to isolate LT coolers to carry out this job, the Overboard line to be isolated. This job requires staging, Nominal Pipe dia is 400A. Supply cooling water to FWD LT cooler with flexible hose and with minimum load on generator job can be carried out or carry out a black out with Emergency DG onload. Temporary arrangement made to restrict the leak. Pipe section replaced with new spare.","2024-04-30T08:00:00","","Completed","2024-04-23T08:00:00","No","No","No","Internal"]
[null,null,null,null,39420,"27_Thu Mar 14 2024 22:58:31 GMT+0800","2024-03-01T08:00:00","Defect","Ship Staff","Ship Staff Insp.","EGCS system CEMS panel, reading for gas analyzer is not operational.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","CEMS local panel is in initializing mode, unable to perform any function, suspect the system is unable to reboot itself. Sample line cleared and system is made operational.","2024-04-30T08:00:00","","Completed","2024-05-10T08:00:00","No","No","No","Internal"]
[null,null,null,null,49802,"27_Mon Dec 18 2023 16:48:30 GMT+0800","2023-12-02T08:00:00","Defect","Ship Staff","Ship Staff Insp.","LT cooler SW overboard line non return check valve leaking, body is holed.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","LT cooler SW overboard line non return check valve leak arrested with wooden plug Jubilee clip and cement arrangement. Same covered with galvanized sheet and painting carried out.  Spare valve received, same will be replaced at next opportunity, we need to plug Overboard or if Overboard valve is holding, we need to change over LT cooler system to flexible hose and shut down sea chest. Check valve replaced with new spare in Singapore April 24","2024-04-30T08:00:00","DLOT230274","Completed","2024-04-23T08:00:00","No","No","No","Internal"]
[null,null,null,null,64319,"27_Mon Nov 20 2023 05:36:43 GMT+0800","2023-11-15T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Deck seal pump in/out and root - Globe valve not holding\n","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Deck seal pump in/out and root - Globe valve needs renewal,  Spares received at Singapore in Jan 24. We need to shut down both Sea chest valve to carry out this job. LT coolers to be used with flexible hose connection with minimum load. Job to be carried out at suitable opportunity. The operation of deck seal pump is satisfactory without any leakages. Deck seal pump inlet and outlet valves replaced with new spare for both the pumps, remaining is the root valve, same to be performed after sea chest isolation. Root valve overhauled found in good order.\n","2024-04-30T08:00:00","DLOT230274","Completed","2024-04-23T08:00:00","No","No","No","Internal"]
[null,null,null,null,62454,"0_Mon Nov 20 2023 05:43:46 GMT+0800","2023-10-19T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Harbour CSW pump discharge NR valve not holding","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Needs renewal, Spare valve received at Singapore in Jan 24. To change this valve Vessel need to shut down sea water system and change over LT coolers to flexible system. The operational of harbour cooling pump is satisfactory without any leakages, Vessel have standby Main cooling sea water pump for the same purpose. Valve replaced with new spare in Singapore April 24","2024-04-30T08:00:00","DLOT230274","Completed","2024-04-23T08:00:00","No","No","No","Internal"]
[null,null,null,null,47177,"27_Mon Nov 20 2023 05:32:50 GMT+0800","2023-10-19T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Harbour cooling SW pump suction valve body found holed","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Harbour cooling SW pump suction valve hole repaired temporarily by cementing. Vessel have spare valve, same to be renewed at earliest opportunity. Vessel need to shut down sea chest and run the LT coolers with flexible hose. The operation of harbour cooling sea water pump is satisfactory without any leakages. Valve replaced with new spare at Singapore April 24","2024-04-30T08:00:00","DLOT230274 ","Completed","2024-04-23T08:00:00","No","No","No","Internal"]
[null,null,null,null,57620,"27_Sun Jun 18 2023 00:11:55 GMT+0800","2023-06-15T08:00:00","Non Conformity","Ship Staff","Ship Staff Insp.","IG vent valve to atmosphere not operational in auto mode since the positioner is not working","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.2","Medium","","","Positioner to renew. RO -DLOT230137 raised.  ","2024-04-30T08:00:00","RO raised  DLOT 230137","Completed","2024-05-13T08:00:00","No","No","No","Internal"]

{"sheet":"Calc","index":2,"n_rows":28,"n_cols":12,"rows_kept":28,"cut":false,"hidden":true,"merged":[]}
["Def_type","Def_cause","Equipments","VIQrefno","Observer_code"]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,"Dim itemSele As Long"]
[null,null,null,null,null,null,null,null,null,null,null,"   dim startRow as integer"]
[null,null,null,null,null,null,null,null,null,null,null,"   startRow=1"]
[null,null,null,null,null,null,null,null,null,null,null,"        For itemSele = 0 To ListBox1.ListCount - 1"]
[null,null,null,null,null,null,null,null,null,null,null,"        If ListBox1.Selected(itemSele) = True Then"]
[null,null,null,null,null,null,null,null,null,null,null,"        Worksheets(\"WorksheetName\").Range(\"A\" & startRow).Value = ListBox1.List(itemSele)"]
[null,null,null,null,null,null,null,null,null,null,null,"        startRow = startRow + 1"]
[null,null,null,null,null,null,null,null,null,null,null,"        End If"]
[null,null,null,null,null,null,null,null,null,null,null,"        Next"]
[null,null,null,null,null,null,null,null,null,null,null,"Dim LastRowA As String"]
[null,null,null,null,null,null,null,null,null,null,null,"        Dim itemSele As Long"]
[null,null,null,null,null,null,null,null,null,null,null,"       Dim startRow as integer"]
[null,null,null,null,null,null,null,null,null,null,null,"        LastRowA = ActiveSheet.Cells(Rows.count, \"A\").End(xlUp).row"]
[null,null,null,null,null,null,null,null,null,null,null,"        startQue = 0"]
[null,null,null,null,null,null,null,null,null,null,null,"        For itemSele = 0 To ListBox1.ListCount - 1"]
[null,null,null,null,null,null,null,null,null,null,null,"        For startRow = 1 To LastRowA"]
[null,null,null,null,null,null,null,null,null,null,null,"        If Worksheets(\"WorksheetName\").Range(\"A\" & startRow).Value = ListBox1.List(itemSele) Then"]
[null,null,null,null,null,null,null,null,null,null,null,"        ListBox1.Selected(itemSele) = True"]
[null,null,null,null,null,null,null,null,null,null,null,"        Exit For"]
[null,null,null,null,null,null,null,null,null,null,null,"        End If"]
[null,null,null,null,null,null,null,null,null,null,null,"        Next j"]
[null,null,null,null,null,null,null,null,null,null,null,"        Next"]
[null,null,null,null,null,null,null,null,null,null,null,"        End If"]

{"sheet":"Areaofobs","index":3,"n_rows":17,"n_cols":2,"rows_kept":17,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Cargo / Ballast Systems",11]
["Cert. & Docu.",2]
["Communication",6]
["Crew Management",3]
["Emgcy. Systems",13]
["Eng. / Strg. Comp.",14]
["General Appearance",15]
["Ice Opns.",17]
["ISM Related",7]
["ISPS Related",10]
["MARPOL Related",9]
["MLC Related",4]
["Mooring",12]
["Navigation",5]
["Safety / LSA / FFA",8]
["Structural Condn. / WT integrity ",16]

{"sheet":"Vessel_type","index":4,"n_rows":1,"n_cols":2,"rows_kept":1,"cut":false,"hidden":true,"merged":[]}
["Vessel_type","ID"]

{"sheet":"Deficiency_type","index":5,"n_rows":8,"n_cols":3,"rows_kept":8,"cut":false,"hidden":true,"merged":[]}
["TITLE","Type of deficiency_description","ID"]
["Breakdown",null,6]
["Critical Equipment",null,4]
["Defect",null,1]
["Guarantee Claim",null,8]
["Non Conformity",null,2]
["Observation",null,3]
["Other",null,7]

{"sheet":"VIQrefno","index":6,"n_rows":427,"n_cols":3,"rows_kept":427,"cut":false,"hidden":true,"merged":[]}
["VIQ_ref_no","Risk Value of observation","ID"]
["1.1","Low",8243]
["1.10","Low",8252]
["1.11","Low",8253]
["1.12","Low",8254]
["1.13","Low",8255]
["1.14","Low",8256]
["1.15","Low",8257]
["1.16","Low",8259]
["1.17","Low",8260]
["1.18","Low",8261]
["1.19","Low",8262]
["1.2","Low",8244]
["1.20","Low",8263]
["1.21","Low",8265]
["1.22","Low",8266]
["1.23","Low",8267]
["1.24","Low",8268]
["1.25","Low",8269]
["1.26","Low",8270]
["1.3","Low",8245]
["1.4","Low",8246]
["1.5","Low",8247]
["1.6","Low",8248]
["1.7","Low",8249]
["1.8","Low",8250]
["1.9","Low",8251]
["1.99","High",11258]
["10.1","Medium",8461]
["10.10","High",8470]
["10.11","Medium",8471]
["10.12","Very High",8472]
["10.13","Very High",8473]
["10.14","Medium",8474]
["10.15","Low",8475]
["10.16","Very High",8476]
["10.17","Very High",8477]
["10.18","High",8478]
["10.19","Very High",8479]
["10.2","Low",8462]
["10.20","High",8480]
["10.21","Medium",8481]
["10.22","Low",8482]
["10.23","Medium",8483]
["10.24","Low",8484]
["10.25","Very High",8485]
["10.26","High",8486]
["10.27","Medium",8487]
["10.28","Low",8488]
["10.29","Medium",8489]
["10.3","Medium",8463]
["10.30","High",8490]
["10.31","Very High",8491]
["10.32","Very High",8492]
["10.33","High",8493]
["10.34","High",8494]
["10.35","Very High",8495]
["10.36","Very High",8496]
["10.37","Medium",8497]
["10.38","Medium",8498]
["10.39","High",8499]
["10.4","High",8464]
["10.40","Medium",8500]
["10.41","Medium",8501]
["10.42","Medium",8502]
["10.43","Medium",8503]
["10.44","Medium",8504]
["10.45","Very High",8505]
["10.46","High",8506]
["10.47","Medium",8507]
["10.48","High",8508]
["10.49","Medium",8509]
["10.5","Low",8465]
["10.50","High",8510]
["10.51","Low",8511]
["10.52","Medium",8512]
["10.53","Medium",8513]
["10.54","High",8514]
["10.55","Low",8515]
["10.6","Very High",8466]
["10.7","Medium",8467]
["10.8","Medium",8468]
["10.9","Medium",8469]
["10.99","High",8516]
["11.1","High",8420]
["11.10","Medium",8429]
["11.11","Very High",8430]
["11.12","Low",8431]
["11.13","Low",8432]
["11.14","Medium",8433]
["11.15","Low",8434]
["11.16","Low",8435]
["11.17","Low",8436]
["11.2","Medium",8421]
["11.3","Medium",8422]
["11.4","Very High",8423]
["11.5","Medium",8424]
["11.6","Medium",8425]
["11.7","High",8426]
["11.8","Low",8427]
["11.9","Low",8428]
["11.99","High",8437]
["12.1","High",8438]
["12.10","High",8448]
["12.11","High",8449]
["12.12","High",8450]
["12.13","High",8451]
["12.14","High",8452]
["12.15","High",8453]
["12.16","High",8454]
["12.17","High",8455]
["12.18","High",8456]
["12.19","High",8457]
["12.2","High",8439]
["12.20","High",8458]
["12.21","High",8459]
["12.3","High",8441]
["12.4","High",8442]
["12.5","High",8443]
["12.6","High",8444]
["12.7","High",8445]
["12.8","High",8446]
["12.9","High",8447]
["12.99","High",8460]
["2.1","Very High",8296]
["2.1.9","Very High",11259]
["2.10","Medium",8304]
["2.11","Medium",8305]
["2.12","Low",8306]
["2.13","Low",8307]
["2.14","Low",8308]
["2.15","Low",8309]
["2.16","Medium",8310]
["2.2","Medium",8297]
["2.3","High",8295]
["2.4","Medium",8298]
["2.5","Medium",8299]
["2.6","Low",8300]
["2.7","High",8301]
["2.8","High",8302]
["2.9","Medium",8303]
["2.99","High",8311]
["3.1","High",8312]
["3.2","Very High",8313]
["3.3","High",8314]
["3.4","Low",8294]
["3.5","Medium",8315]
["3.6","High",8316]
["3.7","Very High",8317]
["3.8","Very High",8318]
["3.99","High",8319]
["4.1","High",8320]
["4.10","High",8329]
["4.11","Medium",8330]
["4.12","Very High",8331]
["4.13","Very High",8332]
["4.14","Very High",8333]
["4.15","Very High",8334]
["4.16","Very High",8335]
["4.17","Very High",8336]
["4.18","Very High",8337]
["4.19","Low",8338]
["4.2","Medium",8321]
["4.20","Very High",8339]
["4.21","High",8340]
["4.22","Low",8341]
["4.23","High",8342]
["4.24","High",8343]
["4.25","Low",8344]
["4.26","Low",8345]
["4.27","High",8346]
["4.3","Medium",8322]
["4.4","High",8323]
["4.5","Very High",8324]
["4.6","Medium",8325]
["4.7","High",8326]
["4.8","Medium",8327]
["4.9","Medium",8328]
["4.99","High",8347]
["5.1","Very High",8517]
["5.10","High",8526]
["5.11","Low",8527]
["5.12","Medium",8528]
["5.13","High",8529]
["5.14","Very High",8530]
["5.15","Medium",8531]
["5.16","Very High",8532]
["5.17","Very High",8533]
["5.18","High",8534]
["5.19","Medium",8535]
["5.2","Very High",8518]
["5.20","Medium",8536]
["5.21","Medium",8537]
["5.22","High",8539]
["5.23","Very High",8540]
["5.24","Very High",8541]
["5.25","Medium",8542]
["5.26","Medium",8543]
["5.27","Medium",8544]
["5.28","Very High",8545]
["5.29","High",8546]
["5.3","Low",8519]
["5.30","High",8547]
["5.31","High",8548]
["5.32","High",8549]
["5.33","High",8550]
["5.34","Low",8551]
["5.35","Medium",8552]
["5.36","Low",8553]
["5.37","Low",8554]
["5.38","High",8555]
["5.39","Very High",8556]
["5.4","High",8520]
["5.40","Very High",8557]
["5.41","Very High",8558]
["5.42","Medium",8559]
["5.43","High",8560]
["5.44","High",8561]
["5.45","Medium",8564]
["5.46","Medium",8565]
["5.47","Medium",8566]
["5.48","Medium",8567]
["5.5","Low",8521]
["5.6","Low",8522]
["5.7","Medium",8523]
["5.8","Medium",8524]
["5.9","Very High",8525]
["5.99","High",8568]
["6.1","Medium",8348]
["6.10","Low",8357]
["6.11","High",8358]
["6.12","Medium",8359]
["6.13","Low",8360]
["6.14","High",8361]
["6.15","High",8362]
["6.16","Very High",8363]
["6.17","Very High",8364]
["6.18","Medium",8365]
["6.19","Low",8366]
["6.2","High",8349]
["6.20","Medium",8367]
["6.21","High",8368]
["6.22","Medium",8369]
["6.3","Low",8350]
["6.4","High",8351]
["6.5","Medium",8352]
["6.6","Medium",8353]
["6.7","High",8354]
["6.8","High",8355]
["6.9","Low",8356]
["6.99","High",8370]
["7.1","High",8371]
["7.10","High",8380]
["7.11","High",8381]
["7.12","High",8382]
["7.13","Medium",8383]
["7.14","Medium",8384]
["7.15","High",8385]
["7.16","High",8386]
["7.17","High",8387]
["7.2","High",8372]
["7.3","Low",8373]
["7.4","Low",8374]
["7.5","Low",8375]
["7.6","Medium",8376]
["7.7","Low",8377]
["7.8","High",8378]
["7.9","High",8379]
["7.99","High",8388]
["8.1","Very High",8569]
["8.10","Very High",8578]
["8.100","Low",11227]
["8.101","Medium",11228]
["8.102","Low",11229]
["8.103","Low",11230]
["8.104","Low",11231]
["8.105","Medium",11232]
["8.106","Medium",11233]
["8.107","Low",11234]
["8.108","High",11235]
["8.109","Very High",11236]
["8.11","Medium",8579]
["8.110","High",11237]
["8.111","Medium",11238]
["8.112","High",11239]
["8.113","Medium",11240]
["8.114","Low",11241]
["8.115","High",11242]
["8.116","Medium",11243]
["8.117","Medium",11244]
["8.118","Medium",11245]
["8.119","High",11246]
["8.12","Medium",8580]
["8.120","High",11247]
["8.121","Medium",11248]
["8.122","High",11249]
["8.123","High",11250]
["8.124","Low",11251]
["8.125","High",11252]
["8.126","Medium",11253]
["8.127","Medium",11254]
["8.13","Medium",8581]
["8.14","Very High",8582]
["8.15","High",8583]
["8.16","Very High",8584]
["8.17","Low",8585]
["8.18","High",8586]
["8.19","High",8587]
["8.199","High",11255]
["8.2","Medium",8570]
["8.20","Medium",8588]
["8.21","High",8589]
["8.22","Very High",8590]
["8.23","Medium",8591]
["8.24","Medium",8592]
["8.25","Very High",8593]
["8.26","High",8594]
["8.27","Medium",8595]
["8.28","Medium",8596]
["8.29","High",8598]
["8.3","Very High",8571]
["8.30","High",8599]
["8.31","High",8600]
["8.32","Low",8601]
["8.33","Medium",8602]
["8.34","High",8603]
["8.35","Medium",8604]
["8.36","Medium",8605]
["8.37","High",8607]
["8.38","Medium",8608]
["8.39","Medium",8609]
["8.4","Medium",8572]
["8.40","High",8610]
["8.41","Medium",8611]
["8.42","Medium",8612]
["8.43","Very High",8613]
["8.44","High",8615]
["8.45","High",8616]
["8.46","Very High",8617]
["8.47","Very High",8618]
["8.48","Medium",8619]
["8.49","High",8620]
["8.5","Very High",8573]
["8.50","Medium",8621]
["8.51","Low",8622]
["8.52","Low",8623]
["8.53","Low",8624]
["8.54","High",8625]
["8.55","Low",11182]
["8.56","Medium",11183]
["8.57","Medium",11184]
["8.58","High",11185]
["8.59","High",11186]
["8.6","Medium",8574]
["8.60","High",11187]
["8.61","Medium",11188]
["8.62","Very High",11189]
["8.63","High",11190]
["8.64","Medium",11191]
["8.65","Low",11192]
["8.66","High",11193]
["8.67","High",11194]
["8.68","High",11195]
["8.69","Medium",11196]
["8.7","High",8575]
["8.70","Medium",11197]
["8.71","Very High",11198]
["8.72","Medium",11199]
["8.73","Medium",11200]
["8.74","High",11201]
["8.75","Medium",11202]
["8.76","Medium",11203]
["8.77","Medium",11204]
["8.78","Medium",11205]
["8.79","Medium",11206]
["8.8","Medium",8576]
["8.80","Medium",11207]
["8.81","Low",11208]
["8.82","Medium",11209]
["8.83","Low",11210]
["8.84","Low",11211]
["8.85","Medium",11212]
["8.86","Medium",11213]
["8.87","Medium",11214]
["8.88","Low",11215]
["8.89","High",11216]
["8.9","High",8577]
["8.90","High",11217]
["8.91","High",11218]
["8.92","Medium",11219]
["8.93","Low",11220]
["8.94","Low",11221]
["8.95","Medium",11222]
["8.96","Medium",11223]
["8.97","Low",11224]
["8.98","High",11225]
["8.99","Medium",11226]
["9.1","Low",8390]
["9.10","Medium",8399]
["9.11","Medium",8400]
["9.12","Medium",8401]
["9.13","Low",8402]
["9.14","Medium",8403]
["9.15","Medium",8404]
["9.16","High",8405]
["9.17","High",8406]
["9.18","Low",8407]
["9.19","Low",8408]
["9.2","Very High",8391]
["9.20","Medium",8409]
["9.21","Medium",8410]
["9.22","Low",8411]
["9.23","Low",8412]
["9.24","Medium",8413]
["9.25","Low",8414]
["9.26","Low",8415]
["9.27","Low",8416]
["9.28","Medium",8417]
["9.29","Low",8418]
["9.3","Very High",8392]
["9.4","High",8393]
["9.5","High",8394]
["9.6","Low",8395]
["9.7","Medium",8396]
["9.8","Medium",8397]
["9.9","Medium",8398]
["9.99","High",8419]

{"sheet":"Equipment_list","index":7,"n_rows":28,"n_cols":3,"rows_kept":28,"cut":false,"hidden":true,"merged":[]}
["TITLE","Equipment_list_description","ID"]
["Accommodation",null,12]
["Cargo Mach.",null,13]
["Critical Equip.",null,16]
["Deck - Machinery",null,18]
["Deck - Mooring Machinery",null,15]
["Deck - Pipe / Fittings",null,20]
["Documentation",null,21]
["E/R - Air Comp.",null,8]
["E/R - Aux. Engine",null,4]
["E/R - Aux. Mach.",null,7]
["E/R - Boiler",null,5]
["E/R - Main Engine",null,3]
["E/R - Pipes/ valves & fittings",null,9]
["E/R - Pumps",null,32]
["E/R - Purifier",null,6]
["Elect. Mach. & Equip.",null,10]
["Hull & Tanks",null,19]
["Inert Gas",null,14]
["LSA / FFA",null,17]
["Miscellaneous",null,22]
["Navigation - DGPS / EPFS / AIS",null,28]
["Navigation - ECDIS",null,25]
["Navigation - Echo Sounder / Speed Log",null,26]
["Navigation - GMDSS & Communication",null,23]
["Navigation - Others",null,11]
["Navigation - RADAR",null,24]
["Navigation - VDR / BNWAS",null,30]

{"sheet":"PSC_MOU","index":8,"n_rows":11,"n_cols":3,"rows_kept":11,"cut":false,"hidden":true,"merged":[]}
["TITLE","PSC_MOU_description","ID"]
["Asia and the Pacific",null,2]
["Caribbean",null,4]
["Europe and the North Atlantic",null,1]
["Latin America",null,3]
["The Black Sea region",null,6]
["The Indian Ocean",null,8]
["The Mediterranean",null,7]
["The Riyadh MoU",null,9]
["USCG",null,10]
["West and Central Africa",null,5]

{"sheet":"Inspection_type","index":9,"n_rows":13,"n_cols":2,"rows_kept":13,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Bunkering Audit",14]
["Cargo Audit",17]
["Engineering Audit",16]
["ISM Audit",2]
["ISPS Audit",3]
["IT Audit",10]
["MLC Audit",1]
["Mooring Audit",9]
["Nav Audit / Verification",8]
["Onboard Training",18]
["Ship Staff Insp.",15]
["Suptd. Insp.",13]

{"sheet":"Deficiency_Cause","index":10,"n_rows":8,"n_cols":3,"rows_kept":8,"cut":false,"hidden":true,"merged":[]}
["TITLE","Deficiency_Cause_description","ID"]
["Behaviour Based",null,1]
["Equipment Related",null,4]
["External Factors",null,5]
["Human Error",null,7]
["Inappropriate Procedure",null,8]
["Industry Issue",null,6]
["Knowledge Based",null,3]

{"sheet":"Observer_code","index":11,"n_rows":3,"n_cols":3,"rows_kept":3,"cut":false,"hidden":true,"merged":[]}
["TITLE","Observer_code_description","ID"]
["Owner / Marine / Tech. Suptd.",null,3]
["Ship Staff",null,2]

{"sheet":"Status_code","index":12,"n_rows":6,"n_cols":3,"rows_kept":6,"cut":false,"hidden":true,"merged":[]}
["TITLE","Status_code_description","ID"]
["Completed",null,6]
["Deferred to D D",null,5]
["In progress",null,3]
["Not Started",null,2]
["Waiting spare",null,4]

{"sheet":"PSC_ref_no","index":13,"n_rows":19,"n_cols":2,"rows_kept":19,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Alarms",9]
["Cargo operations including equipment",7]
["Certificates & Documentation",2]
["Dangerous Goods",13]
["Emergency Systems",5]
["Fire safety",8]
["ISM",16]
["ISPS",17]
["Life saving appliances",12]
["MLC, 2006",18]
["Other",19]
["Pollution Prevention",15]
["Propulsion and auxiliary machinery",14]
["Radio communication",6]
["Safety of Navigation",11]
["Structural condition",3]
["Water/Weathertight condition",4]
["Working and Living Conditions",10]

{"sheet":"Risk_value_of_obs","index":14,"n_rows":1,"n_cols":2,"rows_kept":1,"cut":false,"hidden":true,"merged":[]}
["Risk Value of observation","ID"]

{"sheet":"Year","index":15,"n_rows":18,"n_cols":1,"rows_kept":18,"cut":false,"hidden":true,"merged":[]}
["Year"]
[2014]
[2015]
[2016]
[2017]
[2018]
[2019]
[2020]
[2021]
[2022]
[2023]
[2024]
[2025]
[2026]
[2027]
[2028]
[2029]
[2030]

{"sheet":"Month","index":16,"n_rows":13,"n_cols":1,"rows_kept":13,"cut":false,"hidden":true,"merged":[]}
["Month"]
["Jan"]
["Feb"]
["Mar"]
["Apr"]
["May"]
["Jun"]
["Jul"]
["Aug"]
["Sep"]
["Oct"]
["Nov"]
["Dec"]

{"sheet":"Date_","index":17,"n_rows":32,"n_cols":1,"rows_kept":32,"cut":false,"hidden":true,"merged":[]}
["Date"]
["01"]
["02"]
["03"]
["04"]
["05"]
["06"]
["07"]
["08"]
["09"]
[10]
[11]
[12]
[13]
[14]
[15]
[16]
[17]
[18]
[19]
[20]
[21]
[22]
[23]
[24]
[25]
[26]
[27]
[28]
[29]
[30]
[31]

{"sheet":"Sheet1","index":18,"n_rows":24,"n_cols":6,"rows_kept":24,"cut":false,"hidden":true,"merged":[]}
[]
[null,"ID","E",null,"Date Recorded",1]
[null,"UNIQUE ID","F",null,"Type of Deficiency",2]
[1,"Date Recorded","G",null,"Observer code",3]
["ignore","Vessel Type","H",null,"Type of Inspection",4]
[null,"Internal / External","I",null,"Description of Deficiency",5]
[null,"Drydock","J",null,"Equipment Categories",6]
[null,"Information Sharing","K",null,"Area of Observation",7]
[null,"Critical_item","L",null,"Deficiency Cause",8]
[null,"Deficiency Type","M",null,"VIQ Ref Number",9]
[null,"Deficiency Cause","N",null,"Risk Value of Obs",10]
[null,"Inspection Type","O",null,"PSC Ref Number",11]
[null,"Equipments","P",null,"PSC MOU ID",12]
[null,"VIQ Reference Number","Q",null,"Action Taken or Required",13]
[null,"Risk Value of the observation","R",null,"Target Date",14]
[null,"PSC Reference Number","S",null,"PO Ref No.",15]
[null,"PSC MOU","T",null,"Status Code",16]
[null,"Observer Code","U",null,"Date Completed",17]
[null,"Target Date","V",null,"Drydock",18]
[null,"Status Code","W",null,"Info Sharing",19]
[null,"Description of Deficiency","X",null,"Critical Item Flag",20]
[null,"Action taken / required","Y",null,"Audit Type",21]
[null,"PO ref no","Z"]
[null,"Date completed","AA"]

{"sheet":"Ship_information","index":19,"n_rows":2,"n_cols":4,"rows_kept":2,"cut":false,"hidden":true,"merged":[]}
["Ship_ID","Ship_Name","FILE_NAME","Export_Date"]
["27","DHT LOTUS (04-03-2024)","27_1711431773388.xlsm","2024-05-13 02:05:75"]

{"sheet":"External_Deficiency_type","index":20,"n_rows":5,"n_cols":3,"rows_kept":5,"cut":false,"hidden":true,"merged":[]}
["TITLE","Type of deficiency_description","ID"]
["Condn of Class / Memo",null,5]
["Defect",null,1]
["Non Conformity",null,2]
["Observation",null,3]

{"sheet":"External_Inspection_type","index":21,"n_rows":11,"n_cols":2,"rows_kept":11,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Cargo Audit",17]
["Flag State Insp.",5]
["ISM Audit",2]
["ISPS Audit",3]
["MLC Audit",1]
["Nav Audit / Verification",8]
["OM Insp. (Eg. SIRE / CDI etc.)",6]
["Others (Eg. Insurance etc.)",12]
["PSC Inspection",4]
["Terminal Insp.",11]

{"sheet":"External_Observer_code","index":22,"n_rows":7,"n_cols":3,"rows_kept":7,"cut":false,"hidden":true,"merged":[]}
["TITLE","Observer_code_description","ID"]
["Class Surveyor",null,4]
["FSC Inspector",null,5]
["Others (Eg. Insurance etc.)",null,9]
["PSC Insp.",null,6]
["SIRE / CDI Insp.",null,8]
["Terminal Insp.",null,7]

{"sheet":"Sheet Version","index":23,"n_rows":2,"n_cols":2,"rows_kept":2,"cut":false,"hidden":true,"merged":[]}
["Version","Title"]
["2.0","Version 2.0"]