{"text_format":"1","workbook":"xlsx","n_sheets":24,"sheets":["Mainsheet","Completed","Calc","Areaofobs","Vessel_type","Deficiency_type","VIQrefno","Equipment_list","PSC_MOU","Inspection_type","Deficiency_Cause","Observer_code","Status_code","PSC_ref_no","Risk_value_of_obs","Year","Month","Date_","Sheet1","Ship_information","External_Deficiency_type","External_Inspection_type","External_Observer_code","Sheet Version"],"not_rendered":{"charts":0,"images":1,"macros":1,"external_links":0,"defined_names":12,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Mainsheet","index":0,"n_rows":41,"n_cols":28,"rows_kept":41,"cut":false,"hidden":false,"merged":[[10,8,10,9],[10,12,10,13],[12,6,12,27],[8,6,8,27]]}
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,"Defect - Damage Monitoring Sheet"]
[]
[null,null,null,null,null,null,null,"Date of Report","05-Jul-2024",null,null,"Ship Name","DHT SCANDINAVIA (08-01-2024)"]
[]
[null,null,null,null,null,null,"VERSION : 2.0"]
[]
[]
[]
[null,null,null,"ID","SHIPSIDE UNIQUEID","UNIQUE ID","Date Recorded","Type of Deficiency","Observer code","Type of Inspection","Description of Deficiency","Equipment Categories","Area of Observation","Deficiency Cause","VIQ Ref Number","Risk Value of Obs","PSC Ref Number","PSC MOU ID","Action Taken or Required","Target Date","PO Ref No.","Status Code","Date Completed","Drydock","Info Sharing","Critical Item","Audit Type","Superintendent Remarks"]
[null,null,null,null,30016,"45_Mon Jan 30 2023 13:57:00 GMT+0800","2023-01-17T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Excess stem dump control valve for atmospheric condenser is malfunctioning.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Diaphragm to be renewed","2024-07-31T08:00:00","SCAN240042","Waiting spare",null,"No","No","No","Internal"]
[null,null,null,null,78942,"45_Sun Oct 01 2023 15:46:24 GMT+0800","2023-09-06T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Aux engine Fuel oil viscosity controller attended by service technician during DD as it was not working. Issue still not resolved.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Presently aux engine fuel oil viscosity is controlled manually by throttling the steam valves. Office has been informed and communication is in process. Makers support requested.","2024-07-31T08:00:00","","In progress",null,"No","No","No","Internal"]
[null,null,null,null,56755,"45_Sun Oct 01 2023 15:49:12 GMT+0800","2023-09-06T08:00:00","Defect","Ship Staff","Ship Staff Insp.","16k-6k steam pressure reducer controller attended by service technician during DD as it was not working. Issue still not resolved.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Presently steam pressure in the line is maintained by manually throttling the inlet valves .  As per last communication with office spares have been ordered under POI SCAN240139. Ref Mail dated 11 May 2024, with Sub DDRL 15 APRIL 2024.","2024-07-31T08:00:00","PO SCAN240139","Waiting spare",null,"No","No","No","Internal"]
[null,null,null,null,33356,"45_Mon Nov 06 2023 08:39:39 GMT+0800","2023-10-25T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Main engine Fuel oil viscosity controller attended by service technician during DD as it was not working. Issue still not resolved.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Trouble shooting in progress / Mail sent to office for further assistance.","2024-07-31T08:00:00","","In progress",null,"No","No","No","Internal"]
[null,null,null,null,62180,"45_Mon Nov 06 2023 15:08:45 GMT+0800","2023-10-30T08:00:00","Observation","Ship Staff","Ship Staff Insp.","A-Deck Public toilet commode is broken from the securing bolt area, same needs to be replaced.","Accommodation","MLC Related","Equipment Related","11.13","Low","","","RO SCAN240022 raised for the same and to be replaced, once received.","2024-07-31T08:00:00","PO # SCAN230298\nPO # SCAN240022","Waiting spare",null,"No","No","No","Internal"]
[null,null,null,null,57231,"45_Fri Nov 17 2023 14:16:47 GMT+0800","2023-11-15T08:00:00","Observation","Ship Staff","Ship Staff Insp.","U-Clamps for Deck piping's for all the Lines are heavily corroded and some are even wasted. Also  Deck Cargo lines , sections touching the supports are rusted & Teflon plates used as barriers are thinned down. ","","Cargo / Ballast Systems","External Factors","11.4","Very High","","","Renewal of wasted U-Clamps and chipping/Painting for the same is in progress.  RO to be raised for additional U-clamps & Teflon sheets as required.","2024-08-31T08:00:00","","In progress",null,"No","No","No","Internal"]
[null,null,null,null,85325,"45_Wed Dec 13 2023 14:16:17 GMT+0800","2023-12-12T08:00:00","Defect","Ship Staff","Ship Staff Insp.","FWG#1 condenser side vapor side end plate found holed and 4 other plates found badly damaged. Temporary repairs carried out to make FWG operational at present. Plates needs to be renewed.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Temporary repairs carried out to make FWG operational at present. Plates needs to be renewed.","2024-07-31T08:00:00","SCAN240048","Waiting spare",null,"No","No","No","Internal"]
[null,null,null,null,56047,"45_Tue Jan 09 2024 19:08:28 GMT+0800","2024-01-09T08:00:00","Defect","Ship Staff","Ship Staff Insp.","BT 1211 - BWTS  No 1  Filter inlet valve not operational in auto and manual mode from the BWTS panel, however it can be opened using emergency hand pump.","Miscellaneous","Cargo / Ballast Systems","Equipment Related","8.11","Medium","","","Trouble shooting  carried out. Found there is a issue with operation of pump as no oil coming of pipeline to the actuator.  Mail has been sent to office for further assistance.","2024-07-31T08:00:00","","In progress",null,"No","No","No","Internal"]
[null,null,null,null,95336,"45_Tue Jan 09 2024 19:12:54 GMT+0800","2024-01-09T08:00:00","Defect","Ship Staff","Ship Staff Insp.","The Ballast and draft gauges in the ccr screen console  all go on error sometimes and need to be reset by removing the fuse and putting it back. ","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.8","Medium","","","Trouble shooting to in progress.","2024-07-30T08:00:00","","In progress",null,"No","No","No","Internal"]
[null,null,null,null,42455,"45_Fri Feb 09 2024 15:01:36 GMT+0800","2024-02-02T08:00:00","Defect","Ship Staff","Ship Staff Insp.","NO 4C cargo tank main valve 123 , was observed to be shutting automatically in neutral position","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.11","Medium","","","Oil loss confirmed from No 4 COT valve actuator body on the opening side. Leak is prominent when valve operated against cargo head (under pressure) , same could not be located with tank entry as valve was operated without any back pressure. RO raised for new actuator as per last communication with office.","2024-07-31T08:00:00","SCAN240165","Waiting spare",null,"No","No","No","Internal"]
[null,null,null,null,48823,"45_Wed Apr 17 2024 07:57:06 GMT+0800","2024-04-08T08:00:00","Defect","Ship Staff","Ship Staff Insp.","No 2 COP vibration monitor found erratic and not giving readings and green light blinking","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.8","Medium","","","it was interchanged with no 1 cop and it was found that sensor was not operational, requisition for the same has been raised SCAN240117 for sensor driver and barrier.","2024-08-30T08:00:00","SCAN240117","Waiting spare",null,"No","No","No","Internal"]
[null,null,null,null,54328,"45_Wed May 22 2024 20:02:41 GMT+0800","2024-05-07T08:00:00","Defect","Ship Staff","Ship Staff Insp.","SCBA Compressor On/Off Breaker found defective during routine inspection.","Elect. Mach. & Equip.","Safety / LSA / FFA","Equipment Related","","","","","As a temporary measure MSB spare breaker used to make SCBA compressor operational.RO raised for new breaker.(RO SCAN240136)","2024-07-31T08:00:00"," SCAN240136","Waiting spare",null,"No","No","No","Internal"]
[null,null,null,null,70340,"45_Sun May 26 2024 20:09:32 GMT+0800","2024-05-11T08:00:00","Defect","Ship Staff","Ship Staff Insp.","ME fuel oil supply pump no 2 coupling is damaged, same temporarily repaired to keep pump stand by.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.3","Medium","","","RO raised. Coupling to be renewed once new spare received.","2024-07-31T08:00:00","SCAN240055","Waiting spare",null,"No","No","No","Internal"]
[null,null,null,null,16478,"45_Sun May 26 2024 20:12:21 GMT+0800","2024-05-10T08:00:00","Defect","Ship Staff","Ship Staff Insp.","No 1 steering gear motor, phase failure relay operates while testing but do not get reset, main breaker needs to be switched off/On to reset same.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.3","Medium","","","The relay needs to be renewed.","2024-07-31T08:00:00","SCAN240073","Waiting spare",null,"No","No","No","Internal"]
[null,null,null,null,98566,"45_Sun May 26 2024 20:24:53 GMT+0800","2024-05-10T08:00:00","Defect","Ship Staff","Ship Staff Insp.","No 2 COT IG pressure reading gets frozen at times. ","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.2","Medium","","","Sensor has been renewed recently. Connections locally and in CCR control unit have been checked, found in order. Vessel has tried rebooting the system. Trobleshooting in progress. ","2024-07-31T08:00:00","","In progress",null,"No","No","No","Internal"]
[null,null,null,null,16871,"45_Sun May 26 2024 20:27:25 GMT+0800","2024-05-13T08:00:00","Defect","Ship Staff","Ship Staff Insp.","PA system mic cable on bridge is damaged and taped. ","Elect. Mach. & Equip.","Safety / LSA / FFA","Equipment Related","10.3","Medium","","","PA system mic cable needs to be renewed.","2024-07-31T08:00:00","SCAN240154","Waiting spare",null,"No","No","No","Internal"]
[null,null,null,null,57375,"45_Sun May 26 2024 20:32:19 GMT+0800","2024-05-06T08:00:00","Defect","Ship Staff","Ship Staff Insp.","LT temperature controller not working in AUTO.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.3","Medium","","","Kongsberg service technician attended at Singapore on 10 June 2024 and reconfigured AMS software. LT controller has been put in to use and system under observation.","2024-07-31T08:00:00","","In progress",null,"No","No","No","Internal"]
[null,null,null,null,31087,"45_Sun May 26 2024 20:37:36 GMT+0800","2024-05-15T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Sea water leak from scrubber gas inlet section.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.3","Medium","","","Leak temporarily repaired by cold work. Material ordered for complete new pipe fabrication in concurrence with office.","2024-07-31T08:00:00","SCAN240102","Waiting spare",null,"No","No","No","Internal"]
[null,null,null,null,96279,"45_Sun May 26 2024 20:48:02 GMT+0800","2024-05-01T08:00:00","Defect","Ship Staff","Ship Staff Insp.","VECS line manifold area has 3 soft patches ","Inert Gas","Cargo / Ballast Systems","Equipment Related","8.28","Medium","","","Discussed with office for further action. RO to be raised for nut/bolts. \nLarge Sections which are not possible to be carried out at sea will be transferred to REFMAN.","2024-08-31T08:00:00","","Not Started",null,"No","No","No","Internal"]
[null,null,null,null,69906,"45_Sun May 26 2024 21:54:57 GMT+0800","2024-05-03T08:00:00","Breakdown","Ship Staff","Ship Staff Insp.","FPK hydraulic Valve is not holding .","Hull & Tanks","Cargo / Ballast Systems","Equipment Related","8.11","Medium","","","Repairs are planned in upcoming week.","2024-07-31T08:00:00","","Not Started",null,"No","No","No","Internal"]
[null,null,null,null,99074,"45_Wed Jun 19 2024 15:31:09 GMT+0800","2024-06-17T08:00:00","Defect","Ship Staff","Ship Staff Insp.","While trying out bosun store hypermist system noticed, pump is stopping after few seconds of running due to faulty pressure switch.","LSA / FFA","Safety / LSA / FFA","Equipment Related","10.30","High","","","Pressure switch has been currently disconnected to ensure continuous running of pump once started and system is working as normal at present.\nVessel has raise RO for new pressure switch under RO SCAN240185.\n\n","2024-07-30T08:00:00","SCAN240185","Waiting spare",null,"No","No","No","Internal"]
[null,null,null,null,69478,"45_Mon Jun 24 2024 17:30:49 GMT+0800","2024-06-23T08:00:00","Observation","Ship Staff","Ship Staff Insp.","Stbd windlass hydraulic brake is not working.","Deck - Mooring Machinery","Mooring","Equipment Related","9.2","Very High","","","Hydraulic cylinder need to be overhauled, internal seals for the piston to be renewed (suspect internal leak). Vessel has spares onboard. Job will be attended shortly.","2024-08-31T08:00:00","","In progress",null,"No","No","No","Internal"]
[null,null,null,null,95031,"45_Thu Jul 04 2024 17:32:28 GMT+0800","2024-07-04T08:00:00","Breakdown","Ship Staff","Ship Staff Insp.","Ref Email Dated 03rd July 2024 , Inlet pipe just below NO.2 BWTS Filter in pump room has developed a hole. Upon further inspection of the filter body & pipe, \n2 more soft patches were also noticed from the inner side of the filter body.\nDe-rusting and surface preparation was carried out. As discussed with office, vessel has carried out 4 coats of cold repairs on the hole and soft patches. \nInterguard paint has been applied on the spots and the entire filter body has been has been painted from the inner side.\n","Cargo Mach.,Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","6.21","High","","","Permanent repairs to be carried out .","2024-09-30T08:00:00","","In progress",null,"No","No","No","Internal"]
[null,null,null,null,73078,"45_Thu Jul 04 2024 17:36:25 GMT+0800","2024-07-04T08:00:00","Breakdown","Ship Staff","Ship Staff Insp.","Ref to email dated 02nd July 2024,. P/R Bulkhead Master v/v No. 204  & Suction v/v No. 223 for No.1 COP / Cargo line  were found to be not holding although\nboth valves were showing full shut indication locally as well as on CCR panel. There are no external leaks. \n","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.11","Medium","","","Seat Rings to be replaced during Next Ballast Voyage. Vessel has Spare seat rings on board.","2024-08-31T08:00:00","","Not Started",null,"No","No","No","Internal"]

{"sheet":"Completed","index":1,"n_rows":940,"n_cols":28,"rows_kept":940,"cut":false,"hidden":false,"merged":[[10,8,10,9],[10,12,10,13],[12,6,12,27],[8,6,8,27]]}
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,"Defect - Damage Monitoring Sheet"]
[]
[null,null,null,null,null,null,null,"Date of Report","05-Jul-2024",null,null,"Ship Name","DHT SCANDINAVIA (08-01-2024)"]
[]
[null,null,null,null,null,null,"VERSION : 2.0"]
[]
[]
[]
[null,null,null,"ID","SHIPSIDE UNIQUEID","UNIQUE ID","Date Recorded","Type of Deficiency","Observer code","Type of Inspection","Description of Deficiency","Equipment Categories","Area of Observation","Deficiency Cause","VIQ Ref Number","Risk Value of Obs","PSC Ref Number","PSC MOU ID","Action Taken or Required","Target Date","PO Ref No.","Status Code","Date Completed","Drydock","Info Sharing","Critical Item","Audit Type","Superintendent Remarks"]
[null,null,null,180,null,"45_Mon Oct 07 2019 02:34:48 GMT+0000","2018-12-29T23:59:35","Defect","Ship Staff","Ship Staff Insp.","DG LO purifier motor found with abnormal sound while running","E/R - Purifier","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Motor overhauled , bearings renewed,working satisfactory.JOB ORDER NO : (V-SCAN017100/19)","2018-12-30T23:59:35","","Completed","2018-12-30T23:59:35","No","No","No","Internal"]
[null,null,null,181,null,"45_Sat Oct 05 2019 23:29:13 GMT+0000","2018-12-30T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Window wiper ( No.2 Stbd side)  found not working ","Navigation - Others","Navigation","Equipment Related","12.1","High","","","Carriage plate renewed with new spare, working satifactory.JOB ORDER NO : (V-SCAN017039/19) ","2019-01-01T23:59:35","","Completed","2019-01-01T23:59:35","No","No","No","Internal"]
[null,null,null,182,null,"45_Mon Oct 07 2019 02:41:53 GMT+0000","2019-01-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Main air compressor#2 auto unloading valve found not operating ","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Renewed with spare valve, working satisfactory .JOB ORDER NO :(V-SCAN 017040/19)","2019-01-02T23:59:35","","Completed","2019-01-02T23:59:35","No","No","No","Internal"]
[null,null,null,194,null,"45_Mon Oct 07 2019 02:49:00 GMT+0000","2019-01-14T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Main engine fuel oil pressure transmitter found malfunctioning ( showing IFL & fluctuating frequently)","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Pressure transmitter renewed with new spare ,wiring checked, found working satisfactory.JOB ORDER NO :(V-SCAN017266/19)","2019-01-14T23:59:35","","Completed","2019-01-14T23:59:35","No","No","No","Internal"]
[null,null,null,183,null,"45_Mon Oct 07 2019 04:47:07 GMT+0000","2019-01-19T23:59:35","Defect","Ship Staff","Ship Staff Insp.","AE#2 auto start malfunctioning. AE#2 starting in auto except when it is in block condition ,while AE#3 starting/running ","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Hyundai technician attended job at Singapore on 14/03/2019 . Found short circuit on cable from instrument panel to junction box. Same to be renewed. Temporarily shorting cables disconnected. Plan to swap the cable between No 1 & No 2 AE and test (18 Mar 2019). Spare cable to be arranged through Hyundai. Reqn pending.","2019-05-23T23:59:35","SCAN190058","Completed","2019-07-01T23:59:35","No","No","No","Internal"]
[null,null,null,184,null,"45_Sat Oct 05 2019 23:54:50 GMT+0000","2019-01-26T23:59:35","Defect","Ship Staff","Ship Staff Insp.","STBD Bridge Wing Rudder Angle Indicator Dimmer Not Working","Navigation - Others","","Equipment Related","8.12","Medium","","","Renewed with new spare PCB ,working satisfactory.unplaned job order no : V-SCAN018052/19","2019-02-27T23:59:35","SCAN190013","Completed","2019-03-04T23:59:35","No","No","No","Internal"]
[null,null,null,185,null,"45_Sat Oct 05 2019 23:46:18 GMT+0000","2019-02-02T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Angle indcator units for Port & Stbd gangways found damaged","Deck - Pipe / Fittings","General Appearance","Equipment Related","5.47","Medium","","","Fabricated new angle indicator units and renewed for both Port and Stbd gangways.","2019-02-07T23:59:35","","Completed","2019-02-05T23:59:35","No","No","No","Internal"]
[null,null,null,186,null,"45_Sat Oct 05 2019 23:33:31 GMT+0000","2019-02-04T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Deck seal water pressure switch found defective and giving alarm","Inert Gas","Cargo / Ballast Systems","Equipment Related","8.35","Medium","","","Renewed with new pressure switch of same range . RO raised for spare. JOB ORDER NO: (V-SCAN017516/19)","2019-02-08T23:59:35","SCAN190020","Completed","2019-02-04T23:59:35","No","No","No","Internal"]
[null,null,null,187,null,"45_Sat Oct 05 2019 23:39:08 GMT+0000","2019-02-04T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Analyse Pump for Fix gas detection systm for ballast tank giving abnormal sound.","Miscellaneous","Cargo / Ballast Systems","Equipment Related","5.21","Medium","","","Pump overhauled and Pump Diaphragm renewed. Pump tested and working satisfactory.JOB ORDER NO :(V-SCAN017523/19)","2019-02-07T23:59:35","","Completed","2019-02-04T23:59:35","No","No","No","Internal"]
[null,null,null,188,null,"45_Sun Oct 06 2019 00:22:06 GMT+0000","2019-02-05T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Acetylene pipe line above paint locker found with material wastage and holed at clamping area","Deck - Pipe / Fittings","General Appearance","Equipment Related","5.26","Medium","","","Wasted section renewed. System tested for leakage and found satisfactory.","2019-03-13T23:59:35","","Completed","2019-03-18T23:59:35","No","No","No","Internal"]
[null,null,null,189,null,"45_Sat Oct 05 2019 23:51:08 GMT+0000","2019-02-13T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Ullage and IG pressure feed not displayed for 1S COT in SAAB Radar console in CCR","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.12","Medium","","","SAAB radar cover opened for 1S COT, found ingress of water. Same cleaned. Wire found core found broken in TGU unit. Same repaired.Working satisfactory now","2019-02-20T23:59:35","","Completed","2019-02-15T23:59:35","No","No","No","Internal"]
[null,null,null,190,null,"45_Sun Oct 06 2019 19:06:37 GMT+0000","2019-02-18T23:59:35","Defect","Ship Staff","Ship Staff Insp.","At middle part of the Port gangway (joint) found some wastage (holes) on the gangway frame body due to corrosion.","Deck - Machinery","General Appearance","Equipment Related","5.47","Medium","","","Wastage built up by steel putty and boxed back. Permanent job to be done at DD. Shall include in Refman. Included in DD spec. REFMAN Export ID: SDR 16 DK.18 09-MAR-2019","2019-02-20T23:59:35","","Completed","2019-06-06T23:59:35","No","No","No","Internal"]
[null,null,null,9426,null,"45_03/01/2020 8:33:15 PM","2019-03-01T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","dynamic data in AIS was not updated to \"moored\" after vessel's berthing","Navigation - GMDSS & Communication","Navigation","Behaviour Based,Human Error","","","","","dynamic data updated","2019-04-07T23:59:35","","Completed","2019-03-01T23:59:35","No","No","No","Internal"]
[null,null,null,9427,null,"45_03/01/2020 8:38:44 PM","2019-03-01T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","The Non WGS 84 Datum Chart in South China Sea after Eastern Bank was not identified and noted in the passage plan for the voyage","Navigation - ECDIS","Navigation","Behaviour Based,Human Error","4.2","Medium","","","The Passage Plan was amended and the Non WGS 84 Datum Chart in South China Sea after Eastern Bank was noted in the passage plan for the voyage","2019-03-01T23:59:35","","Completed","2019-03-01T23:59:35","No","No","No","Internal"]
[null,null,null,191,null,"45_Sun Oct 06 2019 00:10:54 GMT+0000","2019-03-09T23:59:35","Defect","Ship Staff","Ship Staff Insp.","AUS discharge valves of COPT #1, 2 & 3 not responding suitably for AUTO unloading operation.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.11","Medium","","","Valve positioners of all three COPs calibrated and set for AUTO unloading operation.","2019-03-13T23:59:35","","Completed","2019-03-11T23:59:35","No","No","No","Internal"]
[null,null,null,192,null,"45_Mon Oct 07 2019 02:57:16 GMT+0000","2019-03-14T23:59:35","Defect","Ship Staff","Ship Staff Insp.","ECR fwd HVAC unit ineffective cooling. Low sucn press and high dish pressures noticed.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Dryer found defective. New dryer fitted and system put to service and found satisfactory.","2019-03-20T23:59:35","","Completed","2019-03-16T23:59:35","No","No","No","Internal"]
[null,null,null,193,null,"45_Mon Oct 07 2019 03:09:52 GMT+0000","2019-03-15T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Leakage from FWG seawater piping. A section of pipe found wasted.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.31","Very High","","","Wasted section of pipe renewed and system put to service and found good.","2019-03-23T23:59:35","","Completed","2019-03-23T23:59:35","No","No","No","Internal"]
[null,null,null,195,null,"45_Mon Oct 07 2019 03:03:04 GMT+0000","2019-03-23T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Emg gen engine RPM indicator needle did not reflect the actual engine rpm.","Critical Equip.,Elect. Mach. & Equip.","Emgcy. Systems","Equipment Related","10.32","Very High","","","Cables cleaned and retightened and found indicator working normal","2019-03-23T23:59:35","","Completed","2019-03-23T23:59:35","No","No","No","Internal"]
[null,null,null,196,null,"45_Mon Oct 07 2019 03:12:38 GMT+0000","2019-03-26T23:59:35","Defect","Ship Staff","Ship Staff Insp.","#1 FWG condenser outlet line holed.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Pipe line to remove and fabricate new one.","2019-04-01T23:59:35","","Completed","2019-03-28T23:59:35","No","No","No","Internal"]
[null,null,null,197,null,"45_Sun Oct 06 2019 00:25:13 GMT+0000","2019-04-06T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Crew laundry drier not working.Bush got damaged","Miscellaneous","MLC Related","Equipment Related","11.16","Low","","","Bush fabricated and renewed.","2019-04-21T23:59:35","","Completed","2019-04-19T23:59:35","No","No","No","Internal"]
[null,null,null,198,null,"45_Sun Oct 06 2019 23:24:55 GMT+0000","2019-04-06T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Ship Staff Insp.","Stbd provision crane luffing cylinder top cover, hyd leak.","Deck - Machinery","Mooring","Equipment Related","8.76","Medium","","","Seal renewed. Tested and found satisfactory.","2019-06-22T23:59:35","SCAN190083","Completed","2019-07-04T23:59:35","No","No","No","Internal"]
[null,null,null,9424,null,"45_03/01/2020 8:25:32 PM","2019-04-07T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Accom. found to be in slight vacuum during cargo operations","E/R - Air Comp.,Miscellaneous","ISM Related","Human Error","5.1","Very High","","","Accom. pressure adjusted to maintain positive pressure inside accomodation","2019-04-07T23:59:35","","Completed","2019-04-07T23:59:35","No","No","No","Internal"]
[null,null,null,9425,null,"45_03/01/2020 8:30:02 PM","2019-04-07T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","1 VHF on bridge was found on 25W instead of 1W","Navigation - GMDSS & Communication","Communication","Behaviour Based,Human Error","","","","","VHF powered down to 1W","2019-04-07T23:59:35","","Completed","2019-04-07T23:59:35","No","No","No","Internal"]
[null,null,null,9428,null,"45_03/01/2020 8:18:38 PM","2019-04-07T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Training of jr. Officer in equipments for temperature & pressure calibration to be carrie dout","Miscellaneous","Cargo / Ballast Systems","Behaviour Based,Human Error,Knowledge Based","8.26","High","","","pressure & temperature calibration training given to junior officers","2019-04-22T23:59:35","","Completed","2019-04-12T23:59:35","No","No","No","Internal"]
[null,null,null,199,null,"45_Mon Oct 07 2019 03:20:06 GMT+0000","2019-04-08T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Sucn Pipe line choked.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Removed pipe section. Cleared the obstruction and fitted back.","2019-04-20T23:59:35","","Completed","2019-04-16T23:59:35","No","No","No","Internal"]
[null,null,null,200,null,"45_Sun Oct 06 2019 19:02:34 GMT+0000","2019-04-13T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Port windlass, brake cyl hyd leak from bottom & top cover.","Deck - Mooring Machinery","Mooring","Equipment Related","9.14","Medium","","","Seal ring renewed. System tested and found satisfactory.","2019-06-09T23:59:35","","Completed","2019-05-27T23:59:35","No","No","No","Internal"]
[null,null,null,201,null,"45_Sun Oct 06 2019 00:27:39 GMT+0000","2019-04-16T23:59:35","Defect","Ship Staff","Ship Staff Insp.","No 3 COP NRV suspected to malfunction.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.11","Medium","","","NRV inspected and found free. PAL JO: V-SCAN018857/19","2019-04-23T23:59:35","","Completed","2019-04-16T23:59:35","No","No","No","Internal"]
[null,null,null,202,null,"45_Sun Oct 06 2019 23:50:59 GMT+0000","2019-04-16T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Stbd hose crane, jerky during luffing operation","Deck - Machinery","Mooring","Equipment Related","8.76","Medium","","","Fulcrum pins to be lubricated. Crane to be operated and checked. Grease applied through lubrication points. Vibration has reduced. In communication with service provider. Crane luff cyl control valve spool inspected and found normal. Greasing routine repeated. Movement observed to be better. Need to operate onload and check. Job included in Refman DD spec.","2019-07-22T23:59:35","","Completed","2019-07-23T23:59:35","No","No","No","Internal"]
[null,null,null,203,null,"45_Sun Oct 06 2019 19:09:18 GMT+0000","2019-04-20T23:59:35","Defect","Ship Staff","Ship Staff Insp.","No 1 COP AUS discharge valve positioner defective.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.11","Medium","","","Feedback linkage to positioner found disconnected. Same fitted and calibrated. Found satisfactory","2019-05-28T23:59:35","","Completed","2019-05-26T23:59:35","No","No","No","Internal"]
[null,null,null,204,null,"45_Mon Oct 07 2019 00:58:18 GMT+0000","2019-04-23T23:59:35","Defect","Ship Staff","Ship Staff Insp.","DGPS PRINTER NOT OPREATIONAL","Navigation - DGPS / EPFS / AIS","Navigation","Equipment Related","4.7","High","","","NEED TO REPLACE THE PRINTER . ( PRINTER HEAD WAS CHANGED AFTER RECEIVING THE SPARE BUT ISSUE NOT SOLVED. NEED TO REPLACE PRINTER UNIT )","2019-08-17T23:59:35","SCAN190093","Completed","2019-08-16T23:59:35","No","No","No","Internal"]
[null,null,null,205,null,"45_Mon Oct 07 2019 03:23:42 GMT+0000","2019-04-25T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Main Air Compressor #2, 2nd stage cyl head stud cracked.","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Compressor inspected. Cracked stud replaced with spare new stud. Tried out and found satisfactory.","2019-04-26T23:59:35","","Completed","2019-04-26T23:59:35","No","No","No","Internal"]
[null,null,null,206,null,"45_Sun Oct 06 2019 00:30:17 GMT+0000","2019-04-30T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Oil leakage from Aft winch hyd control valve block","Deck - Mooring Machinery","Mooring","Equipment Related","9.14","Medium","","","Control valve block removed. Seals renewed. Winch tested and found satisfactory.","2019-05-07T23:59:35","","Completed","2019-05-02T23:59:35","No","No","No","Internal"]
[null,null,null,207,null,"45_Mon Oct 07 2019 03:30:59 GMT+0000","2019-05-05T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Main air compressor #2, Performance below normal.","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","1st and 2nd stage valves inspected. 2nd stage discharge valve plate found broken. Valve overhauled with new spare. Compressor tried out and found satisfactory.","2019-05-06T23:59:35","V-SCAN019477/19","Completed","2019-05-06T23:59:35","No","No","No","Internal"]
[null,null,null,208,null,"45_Mon Oct 07 2019 03:34:06 GMT+0000","2019-05-09T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Pin hole in Seawater piping, soot tank eductor line.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Pipe removed to workshop. Leaky section renewed and fitted back. Tested and found satisfactory.","2019-05-10T23:59:35","V-SCAN019478/19","Completed","2019-05-10T23:59:35","No","No","No","Internal"]
[null,null,null,209,null,"45_Mon Oct 07 2019 03:37:29 GMT+0000","2019-05-16T23:59:35","Defect","Ship Staff","Ship Staff Insp.","AE #1, unit 6 exh temp dropped during operation. ","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Upon trouble shooting found the fuel injector defective. Replaced with spare fuel injector. Tested and found satisfactory.","2019-05-17T23:59:35","V-SCAN019479/19","Completed","2019-05-17T23:59:35","No","No","No","Internal"]
[null,null,null,210,null,"45_Mon Oct 07 2019 03:43:18 GMT+0000","2019-05-19T23:59:35","Defect","Ship Staff","Ship Staff Insp.","FWG Ejector pump shaft seal leaking","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Pump overhauled, seal renewed and tested. Found satisfactory.","2019-05-20T23:59:35","V-SCAN019480/19","Completed","2019-05-19T23:59:35","No","No","No","Internal"]
[null,null,null,211,null,"45_Mon Oct 07 2019 03:48:25 GMT+0000","2019-05-21T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Main & COPT #3 cool SW pump shaft seal leaking.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Shaft seal renewed with spare.","2019-05-28T23:59:35","V-SCAN019802/19","Completed","2019-05-26T23:59:35","No","No","No","Internal"]
[null,null,null,212,null,"45_Sun Oct 06 2019 19:19:06 GMT+0000","2019-05-22T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Fwd spring winch  hyd return line corroded.","Deck - Mooring Machinery","Mooring","Equipment Related","9.14","Medium","","","Oil drained, Section of pipe removed and Shifted to Engine room workshop. Section of pipe cropped and renewed. System tested and found no leak.","2019-06-02T23:59:35","","Completed","2019-05-24T23:59:35","No","No","No","Internal"]
[null,null,null,213,null,"45_Sun Oct 06 2019 19:31:32 GMT+0000","2019-05-22T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Stbd side Gangway securing arrangement found broken","Deck - Machinery","General Appearance","Equipment Related","5.47","Medium","","","permanent repair carried out. ","2019-06-22T23:59:35","","Completed","2019-06-19T23:59:35","No","No","No","Internal"]
[null,null,null,214,null,"45_Sun Oct 06 2019 19:34:32 GMT+0000","2019-05-22T23:59:35","Defect","Ship Staff","Ship Staff Insp.","3 COT no.2 Cow machine found not rotating during cow wash at last discharge port","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.34","High","","","Machine need to be taken out and overhaul & box back. Overhauled and found satisfactory.","2019-06-22T23:59:35","","Completed","2019-06-16T23:59:35","No","No","No","Internal"]
[null,null,null,215,null,"45_Sun Oct 06 2019 19:42:49 GMT+0000","2019-05-22T23:59:35","Defect","Ship Staff","Ship Staff Insp.","4 Port COT no.1 Cow machine drive unit found during cow wash not rotating as per maker","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.34","High","","","It has been planned to over haul Drive unit & box back on passage. Overhauled and found satisfactory.","2019-06-22T23:59:35","","Completed","2019-06-17T23:59:35","No","No","No","Internal"]
[null,null,null,216,null,"45_Mon Oct 07 2019 04:41:05 GMT+0000","2019-05-25T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Galley hot plate low IR","Elect. Mach. & Equip.","General Appearance","Equipment Related","11.16","Low","","","Galley hot plates dismantled to check the condition of wires and switch , brittle wires changed with spare , Hot plate IR measured found below 3 mega ohms . Due to low IR 440 low insulation alarm is getting activated , need to replace with spare . RO SCAN190102","2019-06-22T23:59:35","V-SCAN020093/19","Completed","2019-06-28T23:59:35","No","No","No","Internal"]
[null,null,null,217,null,"45_Sun Oct 06 2019 18:56:59 GMT+0000","2019-05-26T23:59:35","Defect","Ship Staff","Ship Staff Insp.","VDR error","Navigation - VDR / BNWAS","Navigation","Equipment Related","4.7","High","","","VDR error observed was coming due to alarm in the system same rectified working satisfcactory","2019-05-27T23:59:35","","Completed","2019-05-27T23:59:35","No","No","No","Internal"]
[null,null,null,218,null,"45_Mon Oct 07 2019 03:45:42 GMT+0000","2019-05-26T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Hydraphore pipe outlet to engine room found crack","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.31","Very High","","","Pipe section renewed","2019-06-02T23:59:35","V-SCAN019801/19","Completed","2019-05-28T23:59:35","No","No","No","Internal"]
[null,null,null,219,null,"45_Sun Oct 06 2019 23:27:53 GMT+0000","2019-05-26T23:59:35","Defect","Ship Staff","Ship Staff Insp.","FIXED GAS Detection system internal leakage ","Miscellaneous","Cargo / Ballast Systems","Equipment Related","5.21","Medium","","","Pumps overhauled with spare kit. Tested and found satisfactory.","2019-07-07T23:59:35","SCAN190103","Completed","2019-07-07T23:59:35","No","No","No","Internal"]
[null,null,null,220,null,"45_Sun Oct 06 2019 19:00:02 GMT+0000","2019-05-27T23:59:35","Defect","Ship Staff","Ship Staff Insp.","COT NO -5P PRESSURE ERROR ","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.12","Medium","","","COT NO -5P PRESSURE ERROR and eratic readings were coming on display same rectified by dismantaling the pressure sensor; cleaned calibrated and fitted back, working satisfactory ","2019-05-30T23:59:35","V-SCAN019822/19","Completed","2019-05-30T23:59:35","No","No","No","Internal"]
[null,null,null,221,null,"45_Sun Oct 06 2019 19:22:08 GMT+0000","2019-06-05T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Forward air whistle not working","Navigation - Others","Navigation","Equipment Related","4.7","High","","","Whistle inspected and spares kept ready. Working Satisfactory","2019-06-17T23:59:35","V-SCAN019958/19","Completed","2019-06-18T23:59:35","No","No","No","Internal"]
[null,null,null,222,null,"45_Mon Oct 07 2019 08:18:49 GMT+0000","2019-06-05T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Forward Air whistle not working","Navigation - Others","Navigation","Equipment Related","4.7","High","","","Whistle inspected and spares kept ready.","2019-06-17T23:59:35","V-SCANNO19958/19","Completed","2019-06-18T23:59:35","No","No","No","Internal"]
[null,null,null,223,null,"45_Wed Jul 10 2019 05:20:40 GMT+0000","2019-06-05T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","60% LT Cooler inlet elbow stub piece corroded","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Stub piece to renew. At present cold repair carried out. Cooler need to be drained for repairs. Job shall be attended in ballast passage.","2019-07-02T23:59:35","V-SCAN020263/19","Completed","2019-07-05T23:59:35","No","No","No","Internal"]
[null,null,null,224,null,"45_Mon Oct 07 2019 03:56:51 GMT+0000","2019-06-08T23:59:35","Defect","Ship Staff","Ship Staff Insp.","#2 Boiler FO pump seal found leaking","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Pump to overhaul.","2019-06-16T23:59:35","V-SCAN001481/18","Completed","2019-06-14T23:59:35","No","No","No","Internal"]
[null,null,null,225,null,"45_Mon Oct 07 2019 06:00:53 GMT+0000","2019-06-09T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Atmospheric condensor sea wateroutlet pipe found pin hole","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","External Factors","10.32","Very High","","","Temporary repair done. Awaiting anchorage to do permant repair. DD spec made.","2019-07-17T23:59:35","DD SPEC","Completed","2019-07-17T23:59:35","Yes","No","No","Internal"]
[null,null,null,226,null,"45_Mon Oct 07 2019 05:29:45 GMT+0000","2019-06-11T23:59:35","Defect","Ship Staff","Ship Staff Insp.","STBD waste water pipe storm valve defective. Pin hole in attached pipe","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","External Factors","10.32","Very High","","","STORM VALVE RENEWED WITH NEW SPARE. Pinhole welded and repaired","2019-06-28T23:59:35","V-SCAN020265/19","Completed","2019-06-28T23:59:35","No","No","No","Internal"]
[null,null,null,227,null,"45_Mon Oct 07 2019 05:27:17 GMT+0000","2019-06-12T23:59:35","Defect","Ship Staff","Ship Staff Insp.","GALLEY DRAIN OVERBOARD STORM VALVE BODY LEAKING. VALVE TO RENEW.","E/R - Pipes/ valves & fittings","","External Factors","6.4","High","","","STORM VALVE RENEWED WITH NEW SPARE","2019-06-28T23:59:35","V-SCAN020264/20","Completed","2019-06-29T23:59:35","No","No","No","Internal"]
[null,null,null,228,null,"45_Mon Oct 07 2019 04:00:42 GMT+0000","2019-06-14T23:59:35","Defect","Ship Staff","Ship Staff Insp.","PORT SIDE BRIDGE WING CAMERA HORIZONENTAL DISTORTION NOTICED ON THE SCREEN AND FLICKERING","Elect. Mach. & Equip.,Miscellaneous","Navigation","Equipment Related","11.16","Low","","","CAMERA DISMENTALED CHECKED FOR LOOSE CONNECTIONS ALL INTACT, FOUND NO BURNED PARTS ON PCB. SYSTEM RESTARTED AFTER CHECKS BUT SAME CONDITION , NEED OFFICE ADVICE ","2019-06-22T23:59:35","","Completed","2019-06-17T23:59:35","No","No","No","Internal"]
[null,null,null,229,null,"45_Mon Oct 07 2019 05:43:18 GMT+0000","2019-06-18T23:59:35","Defect","Ship Staff","Ship Staff Insp.","FWG-2  Distallate pump moror windings found open ckt.","E/R - Aux. Mach.","Eng. / Strg. Comp.","External Factors","10.32","Very High","","","Fabricating a spacer ring to fit the motor to the pump flange. Job in progress. ","2019-07-06T23:59:35","","Completed","2019-07-09T23:59:35","No","No","No","Internal"]
[null,null,null,230,null,"45_Mon Oct 07 2019 00:59:51 GMT+0000","2019-06-21T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Telegraph printer not printing properly","Navigation - Others","Navigation","Equipment Related","4.7","High","","","Movement started logging down in Bridge Bell Book and Req has been raised for defect item.","2019-08-17T23:59:35","SCAN190128","Completed","2019-07-16T23:59:35","No","No","No","Internal"]
[null,null,null,231,null,"45_Mon Oct 07 2019 00:12:33 GMT+0000","2019-06-22T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","5P ballast tank valve indication needle overshoots full open posn and falls to zero position when valve is actually full open.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.13","Medium","","","Local indicator opened up for wrong signal found normal working in range as there is mechanical stopper for the needle. Electronic indicator stop overshooting after adjusting from the PCB and dial adjuster below the indicator. ","2019-08-17T23:59:35","","Completed","2019-08-04T23:59:35","No","No","No","Internal"]
[null,null,null,266,null,"45_Sun Oct 06 2019 23:49:00 GMT+0000","2019-06-28T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","WO Sludge tk, Bilge tank – save all edges corroded/wasted","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","External Factors","6.9","Low","","","Included in REFFMA to carry out at DD","2019-07-11T23:59:35","","Completed","2019-07-11T23:59:35","No","No","No","Internal"]
[null,null,null,173,null,"45_Wed Jul 10 2019 02:02:39 GMT+0000","2019-06-28T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Hose crane Emergency pump for Hoist/Luff operation missing, emergency procedures not tried out","Deck - Machinery","Mooring","Equipment Related","8.5","Very High","","","Spare recieved & closed out","2019-12-22T23:59:35","SCAN190177","Completed","2019-12-17T23:59:35","No","No","No","Internal","Will be supplied in Singapore. Target date revised due to lead time of spares."]
[null,null,null,179,null,"45_Mon Oct 07 2019 05:08:42 GMT+0000","2019-06-28T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ER arrival checklist not updated and signed – pages found blank","Miscellaneous","Eng. / Strg. Comp.","External Factors,Human Error","4.3","Medium","","","Checklists are supposed to be diligently followed and updated and it’s a NC – for not following SMS procdures","2019-07-04T23:59:35","","Completed","2019-06-28T23:59:35","No","No","No","Internal"]
[null,null,null,232,null,"45_Mon Oct 07 2019 04:53:26 GMT+0000","2019-06-28T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Aft engine pit dirty and oily","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.19","Very High","","","To clean, check source of leakage and maintain clean.Cleaned and made dry.","2019-08-04T23:59:35","","Completed","2019-06-29T23:59:35","No","No","No","Internal"]
[null,null,null,233,null,"45_Mon Oct 07 2019 08:28:37 GMT+0000","2019-06-28T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ER arrival Checklist not updated and signed pages found blank\t\t","Documentation","Cert. & Docu.","Human Error","8.104","Low","","","Checklist are supposed to be diligently followed and updated and its a NC for not following","2019-07-04T23:59:35","","Completed","2019-06-28T23:59:35","No","No","No","Internal"]
[null,null,null,234,null,"45_Mon Oct 07 2019 05:14:38 GMT+0000","2019-06-28T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp."," CFW cooler Inlet elbow leaking from connection pipe weld seam","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related,External Factors","10.32","Very High","","","To plan for welding repairs at suitable opportunity","2019-09-04T23:59:35","V-SCAN020263/19","Completed","2019-07-05T23:59:35","No","No","No","Internal"]
[null,null,null,235,null,"45_Sun Oct 06 2019 21:28:41 GMT+0000","2019-06-28T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","No spare foam nozzle retaining springs","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.35","Medium","","","Vessel have spare  4 sets","2019-07-18T23:59:35","","Completed","2019-06-29T23:59:35","No","No","No","Internal"]
[null,null,null,236,null,"45_Sun Oct 06 2019 21:34:02 GMT+0000","2019-06-28T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","IG drain line has soft patch","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","11.4","Very High","","","If opening flange to flange section is not possible, then to include in REFFMAN - Shifted to REFMAN","2019-07-18T23:59:35","","Completed","2019-07-03T23:59:35","No","No","No","Internal"]
[null,null,null,237,null,"45_Mon Oct 07 2019 05:33:07 GMT+0000","2019-06-28T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Control air line to LT cooler 3 way valve actuator cylinder leaking","E/R - Aux. Engine","Eng. / Strg. Comp.","External Factors","10.32","Very High","","","To check and rectify. //Gasket renewed.","2019-07-04T23:59:35","","Completed","2019-07-06T23:59:35","No","No","No","Internal"]
[null,null,null,238,null,"45_Mon Oct 07 2019 05:35:05 GMT+0000","2019-06-28T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","FO heater #1, steam line outlet steam trap leaking from gasket","E/R - Main Engine","Eng. / Strg. Comp.","External Factors","10.32","Very High","","","To rectify the leakage. Replaced gasket and rectified","2019-07-18T23:59:35","","Completed","2019-07-07T23:59:35","No","No","No","Internal"]
[null,null,null,239,null,"45_Mon Oct 07 2019 05:37:31 GMT+0000","2019-06-28T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","1 Frdge compressor running with sump oil level low","E/R - Aux. Mach.","Eng. / Strg. Comp.","External Factors","10.32","Very High","","","To top up oil to correct level. // Topped up.","2019-07-11T23:59:35","","Completed","2019-06-29T23:59:35","No","No","No","Internal"]
[null,null,null,240,null,"45_Mon Oct 07 2019 05:40:04 GMT+0000","2019-06-28T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Incinerator Noticed wrapped with cloth on sludge burner pump","E/R - Aux. Mach.","Eng. / Strg. Comp.","External Factors","10.32","Very High","","","Gaskets renewed. No leak observed.","2019-07-18T23:59:35","","Completed","2019-07-07T23:59:35","No","No","No","Internal"]
[null,null,null,241,null,"45_Sun Oct 06 2019 23:32:14 GMT+0000","2019-06-28T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","WBT valves opening hyd line on deck – cross deck line support back plates are wasted at few locations","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.5","Medium","","","To include in REFFMAN, to carry out at DD -Shifted to REFMAN","2019-08-04T23:59:35","","Completed","2019-07-07T23:59:35","No","No","No","Internal"]
[null,null,null,242,null,"45_Sun Oct 06 2019 23:41:08 GMT+0000","2019-06-28T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","2 foam monitor, gun/nozzle retaining spring, hanging looses, broken form support base","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.35","Medium","","","Retaining spring has been replace","2019-07-18T23:59:35","","Completed","2019-07-16T23:59:35","No","No","No","Internal"]
[null,null,null,243,null,"45_Sun Oct 06 2019 23:44:09 GMT+0000","2019-06-28T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Few Hyd return lines were reported renewed recently, as same was wasted","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.5","Medium","","","Wasted section Welded with doubler and fitted back, same has been enter in Refman for Permanent renewal","2019-08-04T23:59:35","","Completed","2019-07-18T23:59:35","No","No","No","Internal"]
[null,null,null,244,null,"45_Sun Oct 06 2019 23:46:11 GMT+0000","2019-06-28T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Gangway Lubricator and moisture drain filters seems not carried out – covers were seized","Deck - Machinery","General Appearance","Equipment Related","5.47","Medium","","","Gangway Lubricator and moisture drain filters cleaned/overhaul and box back","2019-07-18T23:59:35","","Completed","2019-07-18T23:59:35","No","No","No","Internal"]
[null,null,null,245,null,"45_Mon Oct 07 2019 05:56:26 GMT+0000","2019-06-28T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Noticed, Deep Freezer for wet garbage kept in dry provision room","Miscellaneous","Eng. / Strg. Comp.","External Factors","10.32","Very High","","","Discussed with Supt as there is no issue for Deep Freezer in present location.","2019-07-11T23:59:35","","Completed","2019-07-11T23:59:35","No","No","No","Internal"]
[null,null,null,246,null,"45_Mon Oct 07 2019 05:59:03 GMT+0000","2019-06-28T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","WO Sludge tk, Bilge tank – save all edges corroded/wasted","Deck - Machinery","Eng. / Strg. Comp.","External Factors","10.32","Very High","","","Included in REFFMA to carry out at DD","2019-07-11T23:59:35","","Completed","2019-07-11T23:59:35","Yes","No","No","Internal"]
[null,null,null,247,null,"45_Sun Oct 06 2019 23:52:56 GMT+0000","2019-06-28T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Steering flat/storage COT, various valve seat rings lying open in cardboard box – prone to heat and damage","Miscellaneous","Cargo / Ballast Systems","Human Error","10.29","Medium","","","To shift to any stores inside accommodation to avoid damage to seat rings, to take inventory of seat rings and maintain list/update PAL. Shifted.","2019-07-18T23:59:35","","Completed","2019-07-10T23:59:35","No","No","No","Internal"]
[null,null,null,248,null,"45_Mon Oct 07 2019 08:38:27 GMT+0000","2019-06-28T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Steering flat/Stowage COT , various valve seat rings lying open in cardboard box\t","Miscellaneous","Eng. / Strg. Comp.","Human Error","10.29","Medium","","","to shift to any store inside accomodation to avoid damage to seat rings, to take inventory","2019-07-18T23:59:35","","Completed","2019-07-10T23:59:35","No","No","No","Internal"]
[null,null,null,249,null,"45_Sun Oct 06 2019 23:56:19 GMT+0000","2019-06-28T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Pumproom Blower damper remote operation cabinet corroded/wasted","Deck - Machinery","General Appearance","External Factors","5.19","Medium","","","Shifted to REFFMAN","2019-07-23T23:59:35","","Completed","2019-07-23T23:59:35","No","No","No","Internal"]
[null,null,null,250,null,"45_Mon Oct 07 2019 06:02:26 GMT+0000","2019-06-28T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","2 FW cooler SW outletconnection flange piece considerable sea water leakage observed","E/R - Aux. Engine","Eng. / Strg. Comp.","External Factors","10.32","Very High","","","To check/remove intermediate section, renew gasket as necessary. Planned for next ballast passage.","2019-09-04T23:59:35","V-SCAN020696/19","Completed","2019-07-29T23:59:35","No","No","No","Internal"]
[null,null,null,251,null,"45_Mon Oct 07 2019 06:06:33 GMT+0000","2019-06-28T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","IGG sea water line filter casing holed and leaking","Inert Gas","Eng. / Strg. Comp.","External Factors","8.3","Very High","","","To remove the casing weld/repair and fit back","2019-08-07T23:59:35","V-SCAN020696/19","Completed","2019-07-31T23:59:35","No","No","No","Internal"]
[null,null,null,252,null,"45_Mon Oct 07 2019 00:55:15 GMT+0000","2019-06-28T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Near Helicopter area, on deck, observed coating damage and paint peel off around/abt 30 sq mtrs area","Miscellaneous","General Appearance","External Factors","11.3","Medium","","","Improper surface preparation, waste of paints – to ensure proper procedure is followed while paint application","2019-08-07T23:59:35","","Completed","2019-08-07T23:59:35","No","No","No","Internal"]
[null,null,null,253,null,"45_Mon Oct 07 2019 01:01:46 GMT+0000","2019-06-28T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Stores/Space spaces Lying haphazard and doesn’t look organized","Miscellaneous","General Appearance","Human Error","5.11","Low","","","To utlize the next long Voyage, to take inventory, update and arrange/organize orderly. Stores and spares neatly arranged.","2019-07-18T23:59:35","","Completed","2019-07-20T23:59:35","No","No","No","Internal"]
[null,null,null,254,null,"45_Mon Oct 07 2019 06:08:38 GMT+0000","2019-06-28T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Control air dryer Defective/In-operational","E/R - Air Comp.","Eng. / Strg. Comp.","External Factors","10.32","Very High","","","New unit INSTALLED AND COMMISSSIONED","2019-08-28T23:59:35","","Completed","2019-08-26T23:59:35","No","No","No","Internal"]
[null,null,null,255,null,"45_Wed Jul 10 2019 06:12:18 GMT+0000","2019-06-28T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Aux Engines Not fitted with Oil max filters yet","E/R - Aux. Engine","Eng. / Strg. Comp.","External Factors","10.32","Very High","","","Fitted for all three DG's  and working satisfactory","2019-08-26T23:59:35","","Completed","2019-08-30T23:59:35","No","No","No","Internal"]
[null,null,null,256,null,"45_Sun Oct 06 2019 19:48:03 GMT+0000","2019-07-02T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","All winch brake band adjusting bolt clearances were not as per maker’s reccommendation","Deck - Mooring Machinery","Mooring","Equipment Related","9.14","Medium","","","Adjusted as per recommended clearance requiered.","2019-07-11T23:59:35","","Completed","2019-07-02T23:59:35","No","No","No","Internal"]
[null,null,null,175,null,"45_Wed Jul 10 2019 02:09:03 GMT+0000","2019-07-02T23:59:35","Defect","Ship Staff","Ship Staff Insp.","5P I.G pressure not showing on SAAB radar screen","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.13","Medium","",""," Pressure sensor  renewed.  Working satisfactory","2019-12-22T23:59:35","SCAN190136","Completed","2019-12-22T23:59:35","No","No","No","Internal","Will be supplied in Singapore.I will be carrying spares with me to Qingdao. Target date revised due to lead time of spares."]
[null,null,null,176,null,"45_Wed Jul 10 2019 02:11:44 GMT+0000","2019-07-08T23:59:35","Defect","Ship Staff","Ship Staff Insp.","5C C.O.T level and I.G pressure not showing on SAAB radar screen and Loadicator","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.13","Medium","",""," TGE unit and Pressure sensor renewed, working satisfactory.","2019-12-22T23:59:35","SCAN190136","Completed","2019-12-22T23:59:35","No","No","No","Internal","I will be carrying spares with me to Qingdao. Target date revised due to lead time of spares."]
[null,null,null,257,null,"45_Mon Oct 07 2019 05:45:27 GMT+0000","2019-07-09T23:59:35","Defect","Ship Staff","Ship Staff Insp.","E/R QMI oil mist detector for Aux. Boiler in fault","Elect. Mach. & Equip.","Eng. / Strg. Comp.","External Factors","10.32","Very High","","","Detector dismentaled for repair cleaned and fitted back but no posstive result need to replace the detector RO SCAN190137","2019-08-07T23:59:35","SCAN190137","Completed","2019-07-10T23:59:35","No","No","No","Internal"]
[null,null,null,258,null,"45_Mon Oct 07 2019 05:48:58 GMT+0000","2019-07-14T23:59:35","Defect","Ship Staff","Ship Staff Insp.","MGPS LOW SEA CHEST CURRENT GETTING ZERO AFTER SETTING ANY VALUE ","Elect. Mach. & Equip.","Eng. / Strg. Comp.","External Factors","10.32","Very High","","","SYSTEM CHECKED FOR LOOSE CONNECTION FOUND ALL INTACT , SYSTEM RESTARTED BUT NO POSSITIVE RESULT , SUSPECTED POWER  AND CONTROL UNIT SAME OPENED AND REAPIRED SYSTEM WORKING SATISFACTORY  RO SCAN190139 MADE FOR FUTURE USE","2019-08-22T23:59:35","SCAN190139","Completed","2019-07-17T23:59:35","No","No","No","Internal"]
[null,null,null,10745,null,"45_04-Mar-20 12:23:35 PM","2019-07-24T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Ballast Sea Chest (BA 033) Valve Leaking","Cargo Mach.","Cargo / Ballast Systems","Equipment Related,External Factors","8.8","Medium","","","Seat ring to to be renewed. Vessel have spare seat ring onboard. Deferred to dry dock. Job created in REFMAN.","2020-08-23T23:59:35","","Completed","2020-07-14T23:59:35","Yes","No","No","Internal","Job to be shifted in Refman."]
[null,null,null,259,null,"45_Mon Oct 07 2019 00:01:24 GMT+0000","2019-07-26T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Seawater flusing valve found leaking","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.35","Medium","","","Replace valve with spare","2019-07-29T23:59:35","V-SCAN020688","Completed","2019-07-28T23:59:35","No","No","No","Internal"]
[null,null,null,260,null,"45_Mon Oct 07 2019 00:53:00 GMT+0000","2019-07-30T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Stbd side Gangway securing one arrangement found sheared","Deck - Machinery","General Appearance","Equipment Related","5.47","Medium","","","Sheared part permanently repaired and fix back","2019-08-07T23:59:35","","Completed","2019-08-05T23:59:35","No","No","No","Internal"]
[null,null,null,261,null,"45_Mon Oct 07 2019 06:10:28 GMT+0000","2019-08-09T23:59:35","Defect","Ship Staff","Ship Staff Insp.","SW leakage from #1 FWG eductor","E/R - Aux. Engine","Eng. / Strg. Comp.","External Factors","10.32","Very High","","","Eductor body found erroded. Need to replace. RO raised for spare SCAN190158. Repaired by brazing. ","2019-10-07T23:59:35","SCAN190158","Completed","2019-08-26T23:59:35","No","No","No","Internal"]
[null,null,null,8148,null,"45_16/12/2019 3:20:31 PM","2019-08-12T23:59:35","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Clean old oil stains near NO.1 boiler supply pump gland packing.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.19","Very High","","","Oil stain cleaned and painted","2019-09-16T23:59:35","","Completed","2019-09-14T23:59:35","No","No","No","Internal"]
[null,null,null,177,null,"45_Wed Jul 10 2019 06:26:06 GMT+0000","2019-09-07T23:59:35","Defect","Ship Staff","Ship Staff Insp.","QMI MIST DETECTOR AUX BOILER NO 1 NOT OPERATIONAL","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","5.35","Medium","","","QMI SENSOR REPLACED WITH NEW SPARE , WORKING SATISFACTORY","2019-12-22T23:59:35","SCAN190137","Completed","2019-12-19T23:59:35","No","No","No","Internal","Will be Supplied in singapore."]
[null,null,null,262,null,"45_Mon Oct 07 2019 01:08:04 GMT+0000","2019-09-10T23:59:35","Defect","PSC Insp.","PSC Inspection","The Last 1 meter of the Vapor piping upstream of the vapor connection must be painted Red/Yellow/Red. The Vapor control piping on board did not meet the required Color Scheme ","Deck - Pipe / Fittings","Cargo / Ballast Systems","Human Error","8.42","Medium","Cargo operations including equipment","","Red colour marking band of 100 mm as required were painted on the Vapour return line manifold same day of the observation.","2019-09-10T23:59:35","","Completed","2019-09-10T23:59:35","No","No","No","External"]
[null,null,null,263,null,"45_Mon Oct 07 2019 06:17:07 GMT+0000","2019-09-10T23:59:35","Defect","PSC Insp.","PSC Inspection","The condition of the ship’s equipment shall not present dangers to the ship or it’s crew. The gasket material around the incinerator door was deteriorated","Miscellaneous","Eng. / Strg. Comp.","External Factors","10.32","Very High","Other","","Replaced Gasket.","2019-09-10T23:59:35","","Completed","2019-09-11T23:59:35","No","No","No","External"]
[null,null,null,264,null,"45_Mon Oct 07 2019 06:15:33 GMT+0000","2019-09-10T23:59:35","Defect","PSC Insp.","PSC Inspection","The condition of the ship and its equipment shall be maintained to conform to the provisions of the current regulations & ensure the ship remains fit to proceed to sea w/o presenting dangers to the ship or persons. The refractory of the incinerator was degraded.","Miscellaneous","Eng. / Strg. Comp.","External Factors","10.32","Very High","Other","","Degraded refractory material restored with suitable refractory material","2019-09-10T23:59:35","","Completed","2019-09-11T23:59:35","No","No","No","External"]
[null,null,null,265,null,"45_Mon Oct 07 2019 01:10:28 GMT+0000","2019-09-10T23:59:35","Defect","PSC Insp.","PSC Inspection","The Tank Overfill alarm requires an audible & visible alarm. The Warning light was not visible during tests.","Elect. Mach. & Equip.","Cargo / Ballast Systems","Equipment Related","8.24","Medium","Alarms","","Replaced Bulb.","2019-09-10T23:59:35","","Completed","2019-09-10T23:59:35","No","No","No","External"]
[null,null,null,267,null,"45_Mon Oct 07 2019 02:00:46 GMT+0000","2019-09-11T23:59:35","Defect","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","The details relating to type and number of navigation equipment had not been completed within the OCIMF VPQ.","Documentation","Cert. & Docu.","Human Error","1.14","Low","","","The details updated in OCIMF VPQ.","2019-09-11T23:59:35","","Completed","2019-09-11T23:59:35","No","No","No","Internal"]
[null,null,null,268,null,"45_Mon Oct 07 2019 06:19:04 GMT+0000","2019-09-12T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","DECK SEAL PUMP #2 MECHANICAL SEAL LEAK","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","PUMP OVERHAULED, MECHANICAL SEAL RENEWED","2019-09-19T23:59:35","","Completed","2019-09-19T23:59:35","No","No","No","Internal"]
[null,null,null,269,null,"45_Mon Oct 07 2019 06:20:41 GMT+0000","2019-09-12T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","AE FO SUPPLY PUMP MECHANICAL SEAL LEAK","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","PUMP OVERHAULED AND MECHANICAL SEAL RENWED. PUMP PUT IN USE NO LEAKS FOUND","2019-09-19T23:59:35","","Completed","2019-09-16T23:59:35","No","No","No","Internal"]
[null,null,null,8092,null,"45_18/12/2019 3:23:34 PM","2019-09-12T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","UPS in steering gear room giving fault alarm","Elect. Mach. & Equip.","General Appearance","Equipment Related","11.1","High","","","UPS to be renewed.RO raaised","2020-09-22T23:59:35","SCAN 200006","Completed","2020-10-21T23:59:35","No","No","No","Internal"]
[null,null,null,8131,null,"45_16/12/2019 3:32:19 PM","2019-09-12T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Calorifier drain valve having minor leakge","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Leak rectified by tightening drain pipe","2019-09-16T23:59:35","","Completed","2019-09-16T23:59:35","No","No","No","Internal"]
[null,null,null,8132,null,"45_16/12/2019 2:41:48 PM","2019-09-12T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","A.E 2 Duplex filter having minor leakage","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.19","Very High","","","Duplex filter change over cock O- rings renewed, leak rectified.","2019-09-17T23:59:35","","Completed","2019-09-15T23:59:35","No","No","No","Internal"]
[null,null,null,8133,null,"45_16/12/2019 2:45:23 PM","2019-09-12T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","A.E 1 Fuel oil regulating valve having minor leakage","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.19","Very High","","","Ther is no leak, oil stain from fuel pipe, cleaned and painted.","2019-09-22T23:59:35","","Completed","2019-09-19T23:59:35","No","No","No","Internal"]
[null,null,null,8134,null,"45_16/12/2019 2:52:46 PM","2019-09-12T23:59:35","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","M.E jacket water piping behind FWG,2 flanges having salt deposits on it.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","",""," Salt deposits cleaned and painted","2019-09-16T23:59:35","","Completed","2019-09-15T23:59:35","No","No","No","Internal"]
[null,null,null,8135,null,"45_16/12/2019 2:57:49 PM","2019-09-12T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","M.E NO.4 unit lagging cover for exhaust manifold has become loose due to broken rivet","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.19","Very High","","","Lagging cover fixed in place  and rivetted","2019-09-18T23:59:35","","Completed","2019-09-16T23:59:35","No","No","No","Internal"]
[null,null,null,8136,null,"45_16/12/2019 4:16:29 PM","2019-09-12T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Following noted in 12.06.123.00.01 - Tool box meeting filed in engine room section for LFI/LET/ SAFETY FLASH etc - not filled up for entire month of september & August verification & updating in PMS after completion of JOB section not filled. ","Documentation","Cert. & Docu.","Human Error","5.1","Very High","",""," All the columns filled up ","2019-09-20T23:59:35","","Completed","2019-09-14T23:59:35","No","No","No","Internal"]
[null,null,null,8137,null,"45_16/12/2019 4:07:29 PM","2019-09-12T23:59:35","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Minor leakage  observed from NO.i&2 pilot pressure gauge connection for steering gear","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Leak rectified by tightening the connections","2019-09-17T23:59:35","","Completed","2019-09-15T23:59:35","No","No","No","Internal"]
[null,null,null,8138,null,"45_16/12/2019 4:02:11 PM","2019-09-12T23:59:35","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","NO.1/2 Boiler circulating pump gauges are incorrect scale","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.19","Very High","","","Boiler water circulating pump suction pressurte equal to the boiler drum pressure, No 1 pump prssure gauges working good, #2 pump pressure gauge renewewd.","2019-09-13T23:59:35","","Completed","2019-09-13T23:59:35","No","No","No","Internal"]
[null,null,null,8139,null,"45_16/12/2019 2:23:29 PM","2019-09-12T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Securing nut for ladder to Main COPT CSW pump observed to be loose","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.15","Low","","","Securing nut tightned","2019-09-17T23:59:35","","Completed","2019-09-12T23:59:35","No","No","No","Internal"]
[null,null,null,8140,null,"45_16/12/2019 2:48:04 PM","2019-09-12T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","AE 1  Fuel oil drain line lagging missing","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.19","Very High","","","Lagging made on drain line","2019-09-16T23:59:35","","Completed","2019-09-13T23:59:35","No","No","No","Internal"]
[null,null,null,8141,null,"45_16/12/2019 2:37:33 PM","2019-09-12T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","No.2  FWG  ejector pump gland leaking from mechanical seal","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","No gland leak, only come condensate water on top of the casing. it has been cleaned and painted.","2019-09-15T23:59:35","","Completed","2019-09-15T23:59:35","No","No","No","Internal"]
[null,null,null,8142,null,"45_16/12/2019 3:01:55 PM","2019-09-12T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","M.E NO.6 Unit jacket cooling water valve having tell tale sign of minor SW leakage","Main Engine ,E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","It is not SW , JCW FW line , no leaks observed, old salt deposits removed and painted.","2019-09-17T23:59:35","","Completed","2019-09-15T23:59:35","No","No","No","Internal"]
[null,null,null,8143,null,"45_16/12/2019 3:05:01 PM","2019-09-12T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","M.E Auto back wash filter change over valve leaking from gland","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.19","Very High","","","Changing over cock , shaft seals, aond o-rings renewed. Leak rectified.","2019-10-23T23:59:35","","Completed","2019-09-15T23:59:35","No","No","No","Internal"]
[null,null,null,8144,null,"45_16/12/2019 3:08:09 PM","2019-09-12T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","NO.1 ME F.O circulating pump pressure gauge connection having minor leake","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.19","Very High","","","Leak mark cleaned and painted.","2019-09-16T23:59:35","","Completed","2019-09-15T23:59:35","No","No","No","Internal"]
[null,null,null,8145,null,"45_16/12/2019 3:11:38 PM","2019-09-12T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","NO.2 HFO Purifier leakage vent line valve having tell tale signs","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.19","Very High","","","Purifier heater Old oil stain cleaned and painted","2019-09-17T23:59:35","","Completed","2019-09-14T23:59:35","No","No","No","Internal"]
[null,null,null,8146,null,"45_16/12/2019 3:14:13 PM","2019-09-12T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","NO.2 Purifier feed 3 way valve having minor leakage sign","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.19","Very High","","","3-Way valve gland tightened & cleaned","2019-09-13T23:59:35","","Completed","2019-09-15T23:59:35","No","No","No","Internal"]
[null,null,null,8147,null,"45_16/12/2019 3:17:03 PM","2019-09-12T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","AUX BOILER NO.2 Fuel oil heater temp thermometer unlegible","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.19","Very High","","","New thermometer fitted","2019-09-18T23:59:35","","Completed","2019-09-14T23:59:35","No","No","No","Internal"]
[null,null,null,8149,null,"45_16/12/2019 3:23:47 PM","2019-09-12T23:59:35","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Port side engine room store stowage rack dont having and stopper bars","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Stopper bars fabricated and fixed","2019-10-22T23:59:35","","Completed","2019-09-12T23:59:35","No","No","No","Internal"]
[null,null,null,8150,null,"45_16/12/2019 3:36:27 PM","2019-09-12T23:59:35","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Recommended to  fit safety gaurd for both hydrophore distill water pump","Miscellaneous,E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.28","Low","","","Gaurds fabricated and fitted.","2019-09-19T23:59:35","","Completed","2019-09-17T23:59:35","No","No","No","Internal"]
[null,null,null,8151,null,"45_16/12/2019 3:27:18 PM","2019-09-12T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","1 no.s chain block in engine room store observed to be with out safety locking plates on hook","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.28","Low","","","Safety locking plate fitted on chain block","2019-09-22T23:59:35","","Completed","2019-09-19T23:59:35","No","No","No","Internal"]
[null,null,null,8152,null,"45_16/12/2019 3:30:09 PM","2019-09-12T23:59:35","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Portable ladders in engine room to be inspected and ID marked","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.28","Low","","","Inspection done and  ID tags fitted","2019-09-22T23:59:35","","Completed","2019-09-18T23:59:35","No","No","No","Internal"]
[null,null,null,8153,null,"45_16/12/2019 3:42:04 PM","2019-09-12T23:59:35","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Door packing for steering gear room entrance door(A 60) requires to be replaced at the bottom area","Miscellaneous,E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.28","Low","","","Door packing replaced ","2019-09-16T23:59:35","","Completed","2019-09-14T23:59:35","No","No","No","Internal"]
[null,null,null,8154,null,"45_16/12/2019 3:45:39 PM","2019-09-12T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Inspection resords and ID tag to be fitted on block and shackle for emergency escape rescue arrangement","Miscellaneous,E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Behaviour Based","10.28","Low","","","ID tags fitted","2019-09-20T23:59:35","","Completed","2019-09-18T23:59:35","No","No","No","Internal"]
[null,null,null,8155,null,"45_16/12/2019 3:48:40 PM","2019-09-12T23:59:35","Critical Equipment","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Gas mask outside of chemical locker to be removed as it does not have expiry date on the catridge","LSA / FFA","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Catridge type mask replaced with disposible masks  ","2019-09-19T23:59:35","","Completed","2019-09-14T23:59:35","No","No","No","Internal"]
[null,null,null,8156,null,"45_16/12/2019 3:52:06 PM","2019-09-12T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Gasket for steam atomising line for NO.1 boiler having minor leak","E/R - Boiler,E/R - Pipes/ valves & fittings","","Equipment Related","10.19","Very High","","","Leak rectified by renewing gasket","2019-09-22T23:59:35","","Completed","2019-09-17T23:59:35","No","No","No","Internal"]
[null,null,null,8157,null,"45_16/12/2019 3:55:49 PM","2019-09-12T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Date of oxygen analyzer calibration prior discharge operation to be update","Inert Gas","Eng. / Strg. Comp.","Equipment Related","8.26","High","","","Date of oxygen analyzer calibration updated ","2019-09-16T23:59:35","","Completed","2019-09-12T23:59:35","No","No","No","Internal"]
[null,null,null,8158,null,"45_16/12/2019 3:59:22 PM","2019-09-12T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Emergency stop IMO symbol to be pasted near Aux engine emergency stop buttons","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.28","Low","","","Emergency stop IMO symbols pasted","2019-09-15T23:59:35","","Completed","2019-09-13T23:59:35","No","No","No","Internal"]
[null,null,null,8159,null,"45_16/12/2019 4:12:16 PM","2019-09-12T23:59:35","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","UMS alarm for NO.2 GE F.O pressure on 13th sept 2019-0021 hrs lt not recorded in rest hour records for duty engineer","Documentation","Cert. & Docu.","Equipment Related","3.3","High","",""," Entry corrected","2019-09-19T23:59:35","","Completed","2019-09-12T23:59:35","No","No","No","Internal"]
[null,null,null,8160,null,"45_18/12/2019 10:24:02 AM","2019-09-12T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Salt deposit observed on bulb of forward liferaft embarkation light and light not working","Elect. Mach. & Equip.","","Equipment Related","11.11","Very High","","","Replaced light, cleaned lamp, applied silicon sealant, gasket","2019-10-12T23:59:35","","Completed","2019-09-14T23:59:35","No","No","No","Internal"]
[null,null,null,8161,null,"45_18/12/2019 10:31:07 AM","2019-09-12T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Water inside light fixture for WIND ALARM on bridge front.","Elect. Mach. & Equip.","General Appearance","Equipment Related","11.1","High","","","Cleaned the fixtures used silicone and applied gaskets.","2019-09-17T23:59:35","","Completed","2019-09-14T23:59:35","No","No","No","Internal"]
[null,null,null,8126,null,"45_16/12/2019 11:04:58 AM","2019-09-13T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Recommend to have close up inspection of Teflon rollers of both gangways as suspect deterioration in condition. Just by rubbing hands on the roller powder is coming out","Deck - Machinery","ISM Related","External Factors","5.47","Medium","","","Close up Inspection carried out & damage found to be only superficial.","2019-12-13T23:59:35","","Completed","2019-09-26T23:59:35","No","No","No","Internal"]
[null,null,null,6271,null,"45_Wed Jul 10 2019 22:41:37 GMT+0000 (Coordinated Universal Time)","2019-09-14T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Whistle for 1 nos SCBA set (Helicopter Equipment) not working","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.43","High","","","On receival of spare, renewed the same & function test carried out, found working satisfactory.","2019-12-23T23:59:35","SCAN 190174","Completed","2019-12-17T23:59:35","No","No","No","Internal","Will be supplied in Qingdao."]
[null,null,null,8093,null,"45_18/12/2019 3:27:43 PM","2019-09-14T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Signai light column not working, Near Boiler all lights not working, Outside Purifier room, Inside purifier room, Inside engine room workshop.","Elect. Mach. & Equip.","General Appearance","Equipment Related","11.9","Low","","","Signal light column lights renewed.Working good.","2020-02-17T23:59:35","RO SCAN 190173","Completed","2020-01-19T23:59:35","No","No","No","Internal","Item ready, will be supplied at next opportunity. Target date revised accordingly."]
[null,null,null,8096,null,"45_Sun May 12 2019 15:09:22 GMT+0000 (Coordinated Universal Time)","2019-09-14T23:59:35","Defect","Owner / Marine / Tech. Suptd.","ISPS Audit","ISPS Audit - Various different drill scenario’s\n\nrequired to be covered as per SSP-12.01 not\n\ncarried out last 1 year","Documentation","ISPS Related","Human Error","7.4","Low","","","Drills as per SSP 12.01 were carried out for the year in the month of September.\n\nAttached ISPS Drills carried out in last 1 year for reference. All joining officers must \n\nfamiliarize themselves with the company's requirement for frequency of Drills.","2019-12-13T23:59:35","","Completed","2019-09-26T23:59:35","No","No","No","Internal"]
[null,null,null,8097,null,"45_Sun May 12 2019 15:16:52 GMT+0000 (Coordinated Universal Time)","2019-09-14T23:59:35","Non Conformity","Owner / Marine / Tech. Suptd.","ISM Audit","Oil Soaked Lagging noted around\n\nF.O Transfer pump suction filter","E/R - Pipes/ valves & fittings","General Appearance","Human Error","10.19","Very High","","","Renewed oil soaked lagging. While cleaning filter  filter casing should be drained of oil prior removing filter element. Oil soaked lagging if found to be renewed immediately.","2019-12-13T23:59:35","","Completed","2019-10-01T23:59:35","No","No","No","Internal"]
[null,null,null,8098,null,"45_Sun May 12 2019 15:27:31 GMT+0000 (Coordinated Universal Time)","2019-09-14T23:59:35","Non Conformity","Owner / Marine / Tech. Suptd.","ISM Audit","Vessel is equipped with Unitor 15H & Fangzhan TH/15 EEBD's. However donning\n\n& maintenance instructions were not included for Fangzhan TH/15 inside Fire training manual and Fire & safety Operational booklet","Documentation","Safety / LSA / FFA","Human Error","5.34","Low","","","Donning Instructions for Fangzhan TH/15 EEBD were inserted in Fire training Manual & safety Operational booklet. Officer made aware of the requirement for inserting the maker's instructions in case of any changes in LSA/FFA equipments. Training imparted to the responsible officer for the informations that should be available inside Fire training Manual & safety Operational booklet\n\nSame to be monitored & verified in future Fire & safety Operational booklet by Master.","2019-12-13T23:59:35","","Completed","2019-09-26T23:59:35","No","No","No","Internal"]
[null,null,null,8099,null,"45_Sun May 12 2019 15:35:31 GMT+0000 (Coordinated Universal Time)","2019-09-14T23:59:35","Defect","Owner / Marine / Tech. Suptd.","ISM Audit","Rubber Insulation Mat was missing in front of Hydraulic starter panel (440v) & L-7 panel (440v) inside forward bosun store.","Elect. Mach. & Equip.","ISM Related","Human Error","10.24","Low","","","All Crew were briefed about the importance of rubber insulation mats near a switch board for their own safety & if any place the mat is found missing this should be brought to notice of \n\nETO immediately. ETO will include in his weekly wet rounds the position of  rubber insulation mats at each electrical panel to avoid such incidence in future.","2019-12-13T23:59:35","","Completed","2019-10-03T23:59:35","No","No","No","Internal"]
[null,null,null,8100,null,"45_Sun May 12 2019 15:53:11 GMT+0000 (Coordinated Universal Time)","2019-09-14T23:59:35","Defect","Owner / Marine / Tech. Suptd.","ISM Audit","Securing shackle for forward life\n\nraft embarkation ladder was observed to be\n\nheavily rusted and difficult to open","LSA / FFA","Safety / LSA / FFA","Human Error","5.27","Medium","","","Securing shackle for forward life\n\nraft embarkation ladder was freed & greased immediately. Company Maintenance schedule to be followed and implemented as per company Requirement  & Industry Standard.","2019-12-14T23:59:35","","Completed","2019-10-02T23:59:35","No","No","No","Internal"]
[null,null,null,8101,null,"45_Sun May 12 2019 16:03:31 GMT+0000 (Coordinated Universal Time)","2019-09-14T23:59:35","Defect","Owner / Marine / Tech. Suptd.","ISM Audit","Paint Drums in paint locker were\n\nobserved to be stored in double stack above the stopper bar.","Miscellaneous","","Human Error","5.46","Medium","","","All crew members were briefed about hazards involved in stowing paint drums in double stack, they were informed about company procedure clearly stating such stowage is not allowed and single stack stowage should be strictly followed in future.","2019-12-13T23:59:35","","Completed","2019-09-26T23:59:35","No","No","No","Internal"]
[null,null,null,8102,null,"45_Sun May 12 2019 16:15:18 GMT+0000 (Coordinated Universal Time)","2019-09-14T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Nav Audit / Verification","Value for Correction for Sea / Swell / Wave response allowance in section-3 - controlling depth calculation in form 12.01.14.021.00 - UKC calculation form were observed to be used as -0.10 Mtrs for all previous ports rather than basis actual anticipated weather.","Documentation","Navigation","Human Error","4.5","Very High","","","Training carried out by Supt for correct procedure to apply correction value. Same will be monitored & verified in future passage plan by Master.\n\n","2019-12-13T23:59:35","","Completed","2019-09-24T23:59:35","No","No","No","Internal"]
[null,null,null,8103,null,"45_Sun May 12 2019 16:20:32 GMT+0000 (Coordinated Universal Time)","2019-09-14T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Mooring Audit","Gear engaging lever disengaging on port side mooring winch number 1&2 due to excessive play.","Deck - Mooring Machinery","Mooring","Human Error","9.14","Medium","","","The locking arrangement for Winch 1 & 2 were aligned and checked for proper operation.","2019-12-12T23:59:35","","Completed","2019-10-02T23:59:35","No","No","No","Internal"]
[null,null,null,8104,null,"45_Sun May 12 2019 16:09:01 GMT+0000 (Coordinated Universal Time)","2019-09-14T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ME Auto back wash filter heating\n\nsteam valve leaking","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Valve gland packing renewed and leakage rectified. Regular checking of leakage and  preventive maintenance to be done in time. ","2019-12-13T23:59:35","","Completed","2019-10-01T23:59:35","No","No","No","Internal"]
[null,null,null,8106,null,"45_15/12/2019 7:06:05 PM","2019-09-14T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Bottom rubber packing for paint locker natural vent missing","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","Human Error","11.7","High","","","Bottom Rubber packing for paint locker was replaced.","2019-09-17T23:59:35","","Completed","2019-12-13T23:59:35","No","No","No","Internal"]
[null,null,null,8107,null,"45_15/12/2019 7:14:31 PM","2019-09-14T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Drums in paint locker stowed in double layer above stopper bar","Accommodation ,Miscellaneous","Cargo / Ballast Systems","Human Error","5.11","Low","","","Drums were removed,secured and stowed properly.All crew members were briefed about hazards involved in stowing paint drums in double stack, they were informed about company procedure clearly stating such stowage is not allowed and single stack stowage should be strictly followed in future.","2019-12-13T23:59:35","","Completed","2019-09-26T23:59:35","No","No","No","Internal"]
[null,null,null,8108,null,"45_15/12/2019 7:47:45 PM","2019-09-14T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Brake indicators of mooring winches observed to be not aligned when brake applied","Deck - Machinery","Mooring","Human Error","9.7","Medium","","","Brake indicators for mooring winches were alligned after tightening the brakes for all the winches","2019-12-13T23:59:35","","Completed","2019-09-20T23:59:35","No","No","No","Internal"]
[null,null,null,8109,null,"45_15/12/2019 7:53:51 PM","2019-09-14T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Key for ‘Emergency generator room Co2 release’ cabinet to be stored at common location","LSA / FFA","Safety / LSA / FFA","Human Error","5.4","High","","","Key for Emergency Generator Room CO2 Release Cabinet was stored in Ships Office and all Crew were made aware about it.","2019-12-13T23:59:35","","Completed","2019-09-17T23:59:35","No","No","No","Internal"]
[null,null,null,8110,null,"45_15/12/2019 7:57:16 PM","2019-09-14T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Inspection records and ID tags for web slings","Miscellaneous","Mooring","Human Error","10.28","Low","","","Inspection Records and ID Tags for Web Slings were made and filed as required.","2019-12-13T23:59:35","","Completed","2019-09-22T23:59:35","No","No","No","Internal"]
[null,null,null,8111,null,"45_Sun Dec 15 2019 20:04:52 GMT+0000 (Coordinated Universal Time)","2019-09-14T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Forward bosun store Bilge overboard discharge to be sealed","Deck - Pipe / Fittings","Cargo / Ballast Systems","Human Error","6.15","High","","","Forward Bosun store Bilge Overboard Discharge were sealed and same inserted in Environmental Seal Log","2019-12-13T23:59:35","","Completed","2019-09-18T23:59:35","No","No","No","Internal"]
[null,null,null,8112,null,"45_Sun Dec 15 2019 20:08:40 GMT+0000 (Coordinated Universal Time)","2019-09-14T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Dresser for IG line on top of 2C COT having minor leakage  ","Inert Gas","Cargo / Ballast Systems","External Factors","8.23","Medium","","","Dresser for IG line on top of 2C COT was tightened and leak stopped.","2019-12-13T23:59:35","","Completed","2019-09-18T23:59:35","No","No","No","Internal"]
[null,null,null,8113,null,"45_Sun Dec 15 2019 20:43:45 GMT+0000 (Coordinated Universal Time)","2019-09-14T23:59:35","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Recommend to fabricate quick release arrangement for embarkation ladder cover or keep a knife standby to remove the cover in minimum time.","LSA / FFA","Safety / LSA / FFA","Human Error","5.47","Medium","","","Knife has been kept standby to remove the embarkation ladder cover in minimum time.","2019-12-13T23:59:35","","Completed","2019-09-22T23:59:35","No","No","No","Internal"]
[null,null,null,178,null,"45_Wed Jul 10 2019 06:33:22 GMT+0000","2019-09-14T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","145 ltr foam fire extinguisher on boiler platform having superficial cracks on the flexible hose","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.42","Medium","","","new extinguisher rcvd. Put in use.","2019-12-23T23:59:35","SCAN 190174","Completed","2019-12-17T23:59:35","No","No","No","Internal","Will be supplied in Qingdao."]
[null,null,null,8114,null,"45_Sun Dec 15 2019 20:45:49 GMT+0000 (Coordinated Universal Time)","2019-09-14T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Shackle for forward embarkation ladder heavily corroded","LSA / FFA","Safety / LSA / FFA","Human Error","5.47","Medium","","","Shackle for forward embarkation ladder was replaced.","2019-12-13T23:59:35","","Completed","2019-09-17T23:59:35","No","No","No","Internal"]
[null,null,null,8115,null,"45_Sun Dec 15 2019 20:48:58 GMT+0000 (Coordinated Universal Time)","2019-09-14T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Port Side Lifeboat Side glass has become translucent","LSA / FFA","Safety / LSA / FFA","External Factors,Human Error","5.29","High","","","Port Side Lifeboat Side Glass has been replaced.","2019-12-13T23:59:35","","Completed","2019-10-12T23:59:35","No","No","No","Internal"]
[null,null,null,8116,null,"45_16/12/2019 9:22:46 AM","2019-09-14T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Bottom wire for safe access to tanker bow walkway missing ","Miscellaneous","General Appearance","Human Error","12.9","High","","","Walkway Wires were checked and inserted were required","2019-12-13T23:59:35","","Completed","2019-09-15T23:59:35","No","No","No","Internal"]
[null,null,null,8117,null,"45_16/12/2019 9:28:47 AM","2019-09-14T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Safety latch for hook of 1 nos chain block is missing & fitted on outside of the hooks ","Miscellaneous","Mooring","Human Error","10.28","Low","","","Safety latches for all chain blocks were checked and renewed as required .","2019-12-13T23:59:35","","Completed","2019-09-22T23:59:35","No","No","No","Internal"]
[null,null,null,8118,null,"45_16/12/2019 9:52:18 AM","2019-09-14T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Few aluminum ladder on deck observed to be without bottom rubber packing","Miscellaneous","General Appearance","Human Error","12.9","High","","","All Aluminium Ladders were checked for their bottom rubber packing and were renewed where required.","2019-12-13T23:59:35","","Completed","2019-10-06T23:59:35","No","No","No","Internal"]
[null,null,null,8119,null,"45_16/12/2019 9:58:26 AM","2019-09-14T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","1 nos dresser coupling on 5C COT having minor leakage","Deck - Pipe / Fittings","Cargo / Ballast Systems","External Factors","8.15","High","","","Dresser coupling was tightened as required , leak was rectified","2019-12-13T23:59:35","","Completed","2019-09-15T23:59:35","No","No","No","Internal"]
[null,null,null,8120,null,"45_16/12/2019 10:00:34 AM","2019-09-14T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","12.06.015.001 – PPE guide in use on board is old version","Documentation","Cert. & Docu.","Human Error","5.5","Low","","","PPE guide was replaced with latest version","2019-12-13T23:59:35","","Completed","2019-09-15T23:59:35","No","No","No","Internal"]
[null,null,null,8121,null,"45_16/12/2019 10:05:05 AM","2019-09-14T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Drug & Alcohol policy pasted in alleyways and common places to be updated with the latest version","Documentation","Cert. & Docu.","Human Error","3.8","Very High","","","Drug & Alcohol policy pasted in alleyways and common places was updated ","2019-12-13T23:59:35","","Completed","2019-09-16T23:59:35","No","No","No","Internal"]
[null,null,null,8122,null,"45_16/12/2019 10:16:14 AM","2019-09-14T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Vessel is provided with Unitor 15H & FANGZHAN TH/15-1 EEBD’s. However donning & maintenance instructions are missing from Fire training Manual and fire & safety operational booklet","LSA / FFA","Safety / LSA / FFA","Human Error","5.15","Medium","","","Donning Instructions for Fangzhan TH/15 EEBD were inserted in Fire training Manual & safety Operational booklet. Officer made aware of the requirement for inserting the maker's instructions in case of any changes in LSA/FFA equipments.","2019-12-13T23:59:35","","Completed","2019-09-26T23:59:35","No","No","No","Internal"]
[null,null,null,8123,null,"45_16/12/2019 10:27:26 AM","2019-09-14T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Securing strap of spare BA set bottle in foam room broken.","LSA / FFA","Safety / LSA / FFA","Human Error","8.65","Low","","","Securing strap replaced & BA set Bottles secured properly.","2019-12-13T23:59:35","","Completed","2019-09-15T23:59:35","No","No","No","Internal"]
[null,null,null,8124,null,"45_16/12/2019 10:39:52 AM","2019-09-14T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Seals for 2 spare fire extinguishers missing","LSA / FFA","Safety / LSA / FFA","Human Error","5.42","Medium","","","Seals for Extinguishers were placed back fot the 2 spare fire Extinguishers.","2019-12-13T23:59:35","","Completed","2019-09-16T23:59:35","No","No","No","Internal"]
[null,null,null,8125,null,"45_16/12/2019 10:51:05 AM","2019-09-14T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Close Indicator for Fire main isolation valve to upper deck not matching with close indicator when fully closed","LSA / FFA","Safety / LSA / FFA","Equipment Related","11.4","Very High","","","Close Indicator for Fire main isolation valve to upper deck was replaced & matched when fully closed.","2019-12-13T23:59:35","","Completed","2019-09-16T23:59:35","No","No","No","Internal"]
[null,null,null,8127,null,"45_16/12/2019 11:11:43 AM","2019-09-14T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Gear engaging lever taper has worn out for port side mooring winch number 1 & 2. Recommend to inspect all","Deck - Machinery","Mooring","External Factors","9.15","Medium","","","The locking arrangement for Winch 1 & 2 were aligned and checked for proper operation.","2019-12-13T23:59:35","","Completed","2019-10-02T23:59:35","No","No","No","Internal"]
[null,null,null,8128,null,"45_16/12/2019 11:15:43 AM","2019-09-14T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Gap in rubber packing of port side upper deck watertight door when fully closed","Accommodation","Structural Condn. / WT integrity ","External Factors","11.6","Medium","","","Rubber packing of Port side upper deck watertight door was replaced and no gaps found.","2019-12-13T23:59:35","","Completed","2019-10-02T23:59:35","No","No","No","Internal"]
[null,null,null,8129,null,"45_16/12/2019 11:21:51 AM","2019-09-14T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","No-3 foam monitor valve hard to open","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.35","Medium","","","No-3 Foam monitor valve was freed up , greasing carried out and found to be free","2019-11-13T23:59:35","","Completed","2019-09-25T23:59:35","No","No","No","Internal"]
[null,null,null,8130,null,"45_16/12/2019 11:41:35 AM","2019-09-14T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Engine room fire isolation valve in foam room has shaft slightly bent making it hard to close the valve.","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.35","Medium","","","On Detailed inspection it was found that the tightness was due to the dryness of the gland, shaft observed to be in prestine condition, the bend was on the indicator of the valve which has been rectified.Required maintainance carried out on  the gland & valve, found to be closing smoothly.","2019-12-13T23:59:35","","Completed","2019-09-27T23:59:35","No","No","No","Internal"]
[null,null,null,6272,null,"45_Wed Jul 10 2019 22:47:16 GMT+0000 (Coordinated Universal Time)","2019-09-23T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","Engine room crane traverse PORT- STBD motor not working","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.28","Low","","","Traverse motor renewed with spare recieved. Working satisfactory","2019-12-08T23:59:35","SCAN190175","Completed","2019-12-07T23:59:35","No","No","No","Internal","Spares being supplied in Qingdao."]
[null,null,null,8094,null,"45_Sun May 12 2019 14:58:55 GMT+0000 (Coordinated Universal Time)","2019-09-29T23:59:35","Defect","Ship Staff","Nav Audit / Verification","In Master-Pilot Information Exchange, while approaching Singapore anchorage with Pilot onboard the number of shackles  and which anchor planned for use at anchorage was not mentioned.","Navigation - Others","Navigation","Human Error","4.3","Medium","","","Responsible officer was briefed on the entry  regarding the number of shackles & which anchor to be used shall be mentioned in the Master-Pilot Information Exchange when vessel is proceeding to anchorage under pilotage. Master carried out briefing of Navigational watchkeepers and appraised them regarding mandatory entries to be made in Master Pilot Information exchange.","2019-12-29T23:59:35","","Completed","2019-10-15T23:59:35","No","No","No","Internal"]
[null,null,null,8095,null,"45_Sun May 12 2019 15:03:04 GMT+0000 (Coordinated Universal Time)","2019-09-29T23:59:35","Defect","Ship Staff","Nav Audit / Verification","Performance of the echo sounder was not tested on all ranges and scales to verify recordings against depths shown on the chart.","Navigation - Echo Sounder / Speed Log","Navigation","Human Error","4.7","High","","","Responsible Officer was briefed by  Master on the requirement for testing the Performance of the echo sounder on all ranges and scales to verify recordings against depths shown on the chart. Master carried out training of all Navigating officers regarding all Navigational equipment check procedures as required by company sms.","2019-12-29T23:59:35","","Completed","2019-10-15T23:59:35","No","No","No","Internal"]
[null,null,null,6269,null,"45_Sat Nov 02 2019 09:53:17 GMT+0000 (Coordinated Universal Time)","2019-10-16T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Observed leakage through fuel back wash  filter change over cock shaft seal while Auxiliary Engines change over to LSMGO","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.1","Medium","","","O-rings/seal rings renwed and leakage rectified.","2019-10-17T23:59:35","","Completed","2019-10-16T23:59:35","No","No","No","Internal"]
[null,null,null,6274,null,"45_Mon Feb 11 2019 12:22:13 GMT+0000 (Coordinated Universal Time)","2019-10-16T23:59:35","Defect","Ship Staff","Ship Staff Insp.","High Wind strobe light infront of Bridge found wasted. Buzzer for the same in CCR not operational.","Elect. Mach. & Equip.","Cargo / Ballast Systems","Equipment Related","4.5","Very High","","","Strobe light renewed. Buzzer in CCR also renewed.","2020-02-16T23:59:35","SCAN190181","Completed","2020-01-17T23:59:35","No","No","No","Internal","Spare will be ready by 6th Jan. TArget date revised accordingly."]
[null,null,null,6270,null,"45_15/11/2019 3:24:49 AM","2019-10-24T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Fresh water generator ejector pump #1 discharge valve SW leaking from the gland.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.31","Very High","","","Complete valve bonnet renewed as parts wasted.","2019-10-28T23:59:35","","Completed","2019-10-25T23:59:35","No","No","No","Internal"]
[null,null,null,6275,null,"45_15/11/2019 3:33:56 AM","2019-10-24T23:59:35","Defect","Ship Staff","Ship Staff Insp.","FWG Ejector pump #1 Mechanical seal leaking","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.31","Very High","","","Pump has been overhauled , Mechanical seal renewed.","2019-10-28T23:59:35","","Completed","2019-10-25T23:59:35","No","No","No","Internal"]
[null,null,null,6276,null,"45_15/11/2019 4:50:40 AM","2019-11-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","During Saturday safety routine observed Portside lifeboat engine was not starting on No.1 battery","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.27","Medium","","","Battery renewed with new spare.","2019-11-02T23:59:35","","Completed","2019-11-02T23:59:35","No","No","No","Internal"]
[null,null,null,6273,null,"45_16/11/2019 2:48:08 PM","2019-11-06T23:59:35","Other","Ship Staff","Ship Staff Insp.","Anemometer was found damaged in Heavy weather","Navigation - Others","Navigation","External Factors","4.2","Medium","","","Vessel has installed spare anemometer available onboard. Requisitons for spare anemometer has been raised in PAL.","2019-11-22T23:59:35","SCAN190193 ANEMOMETER TRANSMITTER 3 CUP TYPE","Completed","2019-11-11T23:59:35","No","No","No","Internal","Understand , job completed."]
[null,null,null,7058,null,"45_Sun Dec 01 2019 11:50:07 GMT+0000 (Coordinated Universal Time)","2019-11-09T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","HFO purifier #2 breakdown due to bearing failure. Bearing & Spindle found damaged","E/R - Purifier","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Service technician attended for the job. Renewed all necessary parts. working satisfactory.","2019-12-07T23:59:35","","Completed","2019-12-06T23:59:35","No","No","No","Internal","Spares will be supplied in China, Qingdao."]
[null,null,null,16129,null,"45_11/12/2020 10:42:26 PM","2019-11-11T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ECGS deck house exit door handle to stencil O/C , also provide baton.","Miscellaneous","General Appearance","Human Error","","","","","ECGS deck house exit door handle stenciled  O/C , also provided baton.","2020-11-21T23:59:35","","Completed","2020-11-17T23:59:35","No","No","No","Internal"]
[null,null,null,8105,null,"45_Mon Aug 12 2019 13:48:56 GMT+0000 (Coordinated Universal Time)","2019-11-11T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Bunker Transfer Plan / Checklist 12.04.08.011.01 Section 7 - Monitoring of H2S/Benzene Vapors : Benzene reading measured by detector tubes shall be mentioned < Min value that can be measured by the specific tube. For example by Gastec tubes Min measurable value is 0.05 ppm, hence in that case benzene shall be mention <0.05 ppm (if no discoloration observed)\n\nUnderstand vessel has kept the Gas tubes as evidence of monitoring. \n\n","Documentation","ISM Related","Human Error","5.23","Very High","","","Corrective Action : Vessel is having Gastec tubes onboard with minimum value of  0.1 ppm. Corrected benzene measured value as <0.1ppm in the checklist. Scanned copy attached.\n\nPreventive action : Responsible officer engineer has been briefed regarding use of Gastec tubes and entries to be made in Checklists.","2020-02-20T23:59:35","","Completed","2019-11-22T23:59:35","No","No","No","Internal"]
[null,null,null,7060,null,"45_Sat Jan 12 2019 17:36:33 GMT+0000 (Coordinated Universal Time)","2019-11-14T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Pump room blower(Port)found with excessive vibration during running","Deck - Machinery","Cargo / Ballast Systems","Equipment Related","5.18","High","","","Blower inspected and found spider coupling damaged . Same renewed.Working satisfactory.","2019-11-19T23:59:35","","Completed","2019-11-17T23:59:35","No","No","No","Internal"]
[null,null,null,7059,null,"45_Sun Dec 01 2019 11:54:32 GMT+0000 (Coordinated Universal Time)","2019-11-21T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","HFO purifier #1 breakdown due to bearing failure, Top bearing , spindle found damaged","E/R - Purifier","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","ALFALAVAL service technician attended the job, purifier overhauled with new spare parts received. Tested and working satisfactory.","2019-12-23T23:59:35","SCAN 190178, SCAN190214","Completed","2019-12-16T23:59:35","No","No","No","Internal","Spares and service is arranged for Singapore. Hence target date revised."]
[null,null,null,9405,null,"45_02/01/2020 11:01:52 AM","2019-11-24T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Ship Staff Insp.","Main Engine FO viscotherm found not working","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.1","Medium","","","Attended during docking and presently working fine.","2021-01-22T23:59:35","SCAN 200004","Completed","2020-11-22T23:59:35","No","No","No","Internal",""]
[null,null,null,174,null,"45_Wed Jul 10 2019 02:04:42 GMT+0000","2019-11-29T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","LT cooling line to AEs, running below AE Gen platform – soft patch and leaking","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","To repair or renew the pipe section during next Dry Dock. Job shifted to refman.","2020-02-12T23:59:35","","Completed","2020-07-12T23:59:35","Yes","No","No","Internal","Job to be attended during docking."]
[null,null,null,9406,null,"45_02/01/2020 11:11:34 AM","2019-12-04T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Ship Staff Insp.","No.1. Boiler pilot burner actuator erratic .","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Actuator renewed with spare received.","2020-02-20T23:59:35","SCAN190226","Completed","2020-01-16T23:59:35","No","No","No","Internal","Spares will be supplied this call Singapore."]
[null,null,null,9402,null,"45_31/12/2019 8:08:17 PM","2019-12-07T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","On boiler FD fan platform, areas which are near the blower duct are in very dirty condition, to clean.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","External Factors","10.29","Medium","","","Cleaned and painted","2020-02-20T23:59:35","","Completed","2019-12-25T23:59:35","No","No","No","Internal"]
[null,null,null,9403,null,"45_31/12/2019 8:04:28 PM","2019-12-07T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Electrical store are on the expansion tank platform to arrange.","Miscellaneous","Eng. / Strg. Comp.","Knowledge Based","10.29","Medium","","","Eklectrical stores arranged ","2020-02-14T23:59:35","","Completed","2020-02-02T23:59:35","No","No","No","Internal"]
[null,null,null,9407,null,"45_03/01/2020 2:52:58 PM","2019-12-07T23:59:35","Observation,Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Bridge air con base plate is completely corroded. To repair.","Miscellaneous","Structural Condn. / WT integrity ","Human Error,Inappropriate Procedure,Knowledge Based","11.8","Low","","","Temporary repairs made, added to Refman for DD repairs","2020-03-07T23:59:35","","Completed","2019-12-25T23:59:35","No","No","No","Internal"]
[null,null,null,9408,null,"45_03/01/2020 3:02:12 PM","2019-12-07T23:59:35","Defect,Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Various bunker tanks man hole door handle is frozen in lifted condition and posing as hazard. TO free up.","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","External Factors,Human Error","11.8","Low","","","Hydroblasted & painted. Verified free movement of handles.","2020-01-22T23:59:35","","Completed","2020-01-07T23:59:35","No","No","No","Internal"]
[null,null,null,9409,null,"45_03/01/2020 3:06:11 PM","2019-12-07T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","VDR junction box base plate on monkey island is mildly corroded. To renew.","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","External Factors,Human Error,Knowledge Based","11.8","Low","","","VDR junction box base plate rust removed and painted.It will be removed during new VDR installation planned.","2020-02-12T23:59:35","","Completed","2020-02-24T23:59:35","No","No","No","Internal"]
[null,null,null,9410,null,"45_31/12/2019 8:12:18 PM","2019-12-07T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Dishwasher is not operational, to order parts.","Accommodation ","Eng. / Strg. Comp.","Equipment Related","11.16","Low","","","New diswasher installed. Working satisfactorily","2020-09-22T23:59:35","SCAN 200005","Completed","2020-10-23T23:59:35","Yes","No","No","Internal","Target date revised due to spares lead time. Same will be supplied during docking"]
[null,null,null,9411,null,"45_31/12/2019 8:17:40 PM","2019-12-07T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Door lock arrangement from funnel to E/R blower platform needs to be repaired.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Plate fabricated and door lock arrangement repaired.","2020-03-20T23:59:35","","Completed","2020-02-25T23:59:35","No","No","No","Internal"]
[null,null,null,9412,null,"45_01/01/2020 6:53:27 PM","2019-12-07T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ME Running hour meter not working. To order.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.37","Medium","","","trouble shooting done presently working good. RO raised for new spare","2020-02-20T23:59:35","","Completed","2019-12-23T23:59:35","No","No","No","Internal"]
[null,null,null,9413,null,"45_03/01/2020 3:10:14 PM","2019-12-07T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Sludge storage tank paint has peeled off. To paint.","Deck - Pipe / Fittings","General Appearance","External Factors,Human Error,Knowledge Based","11.3","Medium","","","Surface preparation carried out & painted.","2020-03-22T23:59:35","","Completed","2020-03-12T23:59:35","No","No","No","Internal"]
[null,null,null,9414,null,"45_01/01/2020 6:58:23 PM","2019-12-07T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","In workshop there is no stopper for pipe storage area. To fabricate.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Knowledge Based","10.28","Low","","","Stopper fabricated and fitted","2020-01-17T23:59:35","","Completed","2020-01-07T23:59:35","No","No","No","Internal"]
[null,null,null,9415,null,"45_31/12/2019 7:58:47 PM","2019-12-07T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Both Air bottle auto drain is leaking and hence kept shut. To overhaul.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Auto drain sOverhauled and kept open","2019-12-22T23:59:35","","Completed","2019-12-12T23:59:35","No","No","No","Internal"]
[null,null,null,9416,null,"45_31/12/2019 8:02:20 PM","2019-12-07T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Ship Staff Insp.","Air compressor, air bottles and air con compressor / motor to soap wash. Found in dirty condition.","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related","","","","","Soap washed & Cleaned","2020-01-07T23:59:35","","Completed","2019-12-11T23:59:35","No","No","No","Internal"]
[null,null,null,9417,null,"45_31/12/2019 8:20:18 PM","2019-12-07T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Main power light in CO2 room for power change over box not working.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.37","Medium","","","Indication Lamp Renewed","2019-12-14T23:59:35","","Completed","2019-12-11T23:59:35","No","No","No","Internal"]
[null,null,null,9420,null,"45_03/01/2020 2:48:19 PM","2019-12-07T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","BA compressor is fixed in place with rope. TO make permanent arrangement.","LSA / FFA","Safety / LSA / FFA","External Factors,Human Error","5.11","Low","","","Permanent arrangement made.","2019-12-22T23:59:35","","Completed","2019-12-10T23:59:35","No","No","No","Internal"]
[null,null,null,9421,null,"45_03/01/2020 3:14:15 PM","2019-12-07T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","No 2 Outer HFO tank save all is not stencilled for its capacity. ","Deck - Pipe / Fittings","General Appearance","External Factors,Human Error,Knowledge Based","11.8","Low","","","Capacity Stenciled","2019-12-12T23:59:35","","Completed","2019-12-10T23:59:35","No","No","No","Internal"]
[null,null,null,9422,null,"45_03/01/2020 3:16:10 PM","2019-12-07T23:59:35","Non Conformity","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Pump room weather tight door packing to renew. Light passing even when door is fully closed.","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","External Factors,Human Error","11.6","Medium","","","Packing renewed","2019-12-22T23:59:35","","Completed","2019-12-22T23:59:35","No","No","No","Internal"]
[null,null,null,9423,null,"45_03/01/2020 3:08:36 PM","2019-12-07T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Ladder outside paint locker is in very dirty condition. To clean and paint.","Deck - Pipe / Fittings","General Appearance","External Factors,Human Error,Inappropriate Procedure,Knowledge Based","11.3","Medium","","","Cleaning of ladders & steps carried out.","2019-12-22T23:59:35","","Completed","2019-12-11T23:59:35","No","No","No","Internal"]
[null,null,null,9404,null,"45_02/01/2020 9:21:59 AM","2019-12-13T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Ship Staff Insp.","During testing of emergency generator found tachometer not working.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.37","Medium","","","Tachometer  renwed. working satisfactory","2020-02-13T23:59:35","SCAN190230","Completed","2020-01-29T23:59:35","No","No","No","Internal"]
[null,null,null,9418,null,"45_02/01/2020 9:15:04 AM","2019-12-13T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Ship Staff Insp.","During saturday routines observed Emergency generator not starting on battery","Elect. Mach. & Equip.","Emgcy. Systems","Equipment Related","10.36","Very High","","","Battery renewed with spare onboard, tested working satisfactory.","2019-12-14T23:59:35","","Completed","2019-12-13T23:59:35","No","No","No","Internal"]
[null,null,null,9419,null,"45_02/01/2020 11:27:07 AM","2019-12-20T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Ship Staff Insp.","During saturday routines ER ventilation fan No.4 flap actuator found leaking and cylinder and end cover material wasted.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.18","High","","","Renewed with sapre actuator onboard. Tested working satisfactory.","2019-12-23T23:59:35","","Completed","2019-12-22T23:59:35","No","No","No","Internal"]
[null,null,null,9592,null,"45_07/01/2012 1:03:59 AM","2019-12-24T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Old supports for the name board on either sides are heavily corroded, new ones to fabricate.","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","External Factors,Inappropriate Procedure","11.8","Low","","","New supports fabricated & fitted","2020-01-24T23:59:35","","Completed","2020-01-02T23:59:35","No","No","No","Internal"]
[null,null,null,9593,null,"45_07/01/2012 1:08:45 AM","2019-12-24T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Bottom Support plate for the MFHF distribution box is wasted. New one to fabricate","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","External Factors,Human Error,Inappropriate Procedure","11.8","Low","","","New Support  fabricated 7 fitted.","2020-01-24T23:59:35","","Completed","2020-01-01T23:59:35","No","No","No","Internal"]
[null,null,null,9595,null,"45_12/01/2020 9:50:49 AM","2019-12-24T23:59:35","Defect","Ship Staff","Ship Staff Insp.","ER vent fan #4 air actuator cylinder body found wasted and air leaking.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Air actuator renewed, tested satisfactory","2019-12-25T23:59:35","","Completed","2019-12-25T23:59:35","No","No","No","Internal"]
[null,null,null,9871,null,"45_17/01/2020 1:36:26 PM","2020-01-08T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Hydraulic leak from the cylinder associated with engaging lever for STBD Windlass","Deck - Mooring Machinery","Mooring","Equipment Related,External Factors","9.2","Very High","","","Cylinder renewed. Leak rectified.","2020-01-12T23:59:35","","Completed","2020-01-09T23:59:35","No","No","No","Internal"]
[null,null,null,10536,null,"45_16/02/2020 8:36:22 PM","2020-01-22T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Lips of Natural Vent flaps rubber packing near China passage corroded.","Accommodation,Miscellaneous","General Appearance","Equipment Related,Human Error","11.1","High","","","De-rusted & painted","2020-04-21T23:59:35","","Completed","2020-04-19T23:59:35","No","No","No","Internal"]
[null,null,null,10537,null,"45_16/02/2020 8:30:34 PM","2020-01-22T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Cover of Dustbins in common spaces found broken.","Critical Equip.,Miscellaneous","General Appearance","Equipment Related,Human Error","6.2","High","","","NEW DUST BINS PUT IN USE","2020-04-21T23:59:35","SCAN200036","Completed","2020-06-09T23:59:35","No","No","No","Internal","WVessel will receive the RO on 6th June."]
[null,null,null,10540,null,"45_16/02/2020 12:05:10 PM","2020-01-24T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Ship Staff Insp.","16 K steam inlet valve bonnet found slightly  leaking (before auto dump valve)","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Steam isolated and valve bonnet gasket renewed.","2020-01-28T23:59:35","","Completed","2020-01-25T23:59:35","No","No","No","Internal"]
[null,null,null,10538,null,"45_16/02/2020 11:33:30 AM","2020-01-26T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Melted grease / Oil collected in the steering gear save all tray. Understand as per ship staff same is from the chain coupling. Grease to renew and confirm leakage.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Coupling grease renewed, no leakages observed.","2020-05-02T23:59:35","","Completed","2020-02-12T23:59:35","No","No","No","Internal"]
[null,null,null,10539,null,"45_16/02/2020 12:01:12 PM","2020-01-26T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ME sump condition to improve by better purification.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.7","Medium","","","LO Purifier tamperature maintained at 95°C, and optumum feed.ME sump oil condition improved.","2020-05-03T23:59:35","","Completed","2020-06-22T23:59:35","No","No","No","Internal"]
[null,null,null,10541,null,"45_16/02/2020 11:44:36 AM","2020-01-26T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Main air bottle, oil marks. Same was reported closed last time but still oil marks are clearly visible.","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Air bottles cleaned and painted","2020-02-13T23:59:35","","Completed","2020-02-04T23:59:35","No","No","No","Internal"]
[null,null,null,10542,null,"45_16/02/2020 11:55:35 AM","2020-01-26T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Water cooler outside ECR dripping continuously.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Water fountain tap repaired and fitted back. not dripping.","2020-03-02T23:59:35","","Completed","2020-02-05T23:59:35","No","No","No","Internal"]
[null,null,null,10543,null,"45_16/02/2020 11:39:37 AM","2020-01-26T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Steering gear door lock to renew.","E/R - Air Comp.,E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Lock removed, repaired and fitted back, working satisfactory","2020-03-02T23:59:35","","Completed","2020-02-05T23:59:35","No","No","No","Internal"]
[null,null,null,10553,null,"45_18/02/2020 5:02:00 PM","2020-01-26T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Both Lifeboat lowering motor and nearby area has rust patches","Deck - Machinery","General Appearance","External Factors","11.1","High","","","de rusted & painted.","2020-05-03T23:59:35","","Completed","2020-05-08T23:59:35","No","No","No","Internal"]
[null,null,null,10555,null,"45_18/02/2020 5:06:47 PM","2020-01-26T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Stbd windlass gear case oil is contaminated with water.","Deck - Mooring Machinery","Mooring","External Factors,Human Error","9.14","Medium","","","Oil Renewed","2020-02-18T23:59:35","","Completed","2020-02-18T23:59:35","No","No","No","Internal"]
[null,null,null,10556,null,"45_18/02/2020 4:57:44 PM","2020-01-26T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Aft mooring winches canvas cover is torn, same to be renewed.","Deck - Mooring Machinery","General Appearance","External Factors","11.1","High","","","Canvas cover renewed","2020-02-19T23:59:35","","Completed","2020-02-07T23:59:35","No","No","No","Internal"]
[null,null,null,10557,null,"45_18/02/2020 5:08:12 PM","2020-01-26T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Fore peak store light fitting top to clean","Deck - Machinery","General Appearance","External Factors,Human Error","11.1","High","","","Cleaned","2020-03-18T23:59:35","","Completed","2020-02-06T23:59:35","No","No","No","Internal"]
[null,null,null,10552,null,"45_18/02/2020 4:59:16 PM","2020-02-03T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Ship Staff Insp.","Emergency CO2 release box for emergency DG is in corroded condition.","Deck - Machinery","General Appearance","External Factors,Human Error","11.1","High","","","Added in Refman for DD Repairs","2020-05-03T23:59:35","","Completed","2020-02-22T23:59:35","No","No","No","Internal","Job to be completed, after joining of fitter."]
[null,null,null,10554,null,"45_18/02/2020 5:03:52 PM","2020-02-03T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Ship Staff Insp.","Foam monitor near isolation valve no 1 leaking from the flange.","Deck - Machinery","General Appearance","External Factors,Human Error","11.1","High","","","Rectified","2020-02-18T23:59:35","","Completed","2020-02-16T23:59:35","No","No","No","Internal"]
[null,null,null,10746,null,"45_03/03/2020 12:11:48 PM","2020-02-14T23:59:35","Defect","Ship Staff","Ship Staff Insp.","During saturday routine test found Port lifeboat was not starting on #2 battery.","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.27","Medium","","","Battery renewed with old good spare battery, working satisfactory. RO wiill be raised for new battery.","2020-02-15T23:59:35","","Completed","2020-02-14T23:59:35","No","No","No","Internal"]
[null,null,null,11339,null,"45_30/03/2020 3:34:52 PM","2020-03-02T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Manifold Drip Tray Grattings need to be Derusted & Fully Painted .","Deck - Pipe / Fittings","General Appearance","External Factors,Human Error","6.2","High","","","Both side manifold gratings derusting & painting completed.","2020-09-22T23:59:35","","Completed","2020-08-28T23:59:35","No","No","No","Internal","Job in progress. Target date revised accordingly."]
[null,null,null,11342,null,"45_30/03/2020 3:42:52 PM","2020-03-02T23:59:35","Observation","Ship Staff","Ship Staff Insp.","E/room Vents found rusted.","Deck - Pipe / Fittings","General Appearance","External Factors,Human Error","6.2","High","","","de-rusted & Painted.","2020-06-02T23:59:35","","Completed","2020-04-19T23:59:35","No","No","No","Internal"]
[null,null,null,11343,null,"45_30/03/2020 3:41:00 PM","2020-03-02T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Funnel Casing found Faded","Deck - Pipe / Fittings","General Appearance","External Factors,Human Error","6.2","High","","","Funnel painting carried out. ","2020-06-02T23:59:35","","Completed","2020-07-10T23:59:35","No","No","No","Internal","Job already completed. Update it."]
[null,null,null,10854,null,"45_20/03/2020 11:57:56 AM","2020-03-04T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Lagging of steam line of OWS is very poorly placed. To renew.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Knowledge Based","10.19","Very High","","","Renewed lagging of OWS heating lines","2020-04-12T23:59:35","","Completed","2020-03-12T23:59:35","No","No","No","Internal"]
[null,null,null,10855,null,"45_20/03/2020 12:12:40 PM","2020-03-04T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Drain box near stbd side of COPT plateform, to clean and paint.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Human Error,Knowledge Based","10.19","Very High","","","cleaned and painted","2020-03-22T23:59:35","","Completed","2020-03-11T23:59:35","No","No","No","Internal"]
[null,null,null,10856,null,"45_20/03/2020 12:21:46 PM","2020-03-04T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Condenser by pass valve to renew. To order new valve","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Valve received .To renew                                                .Old valve eased up . New valve kept as spare                              ","2020-08-23T23:59:35","SCAN 200083","Completed","2020-08-16T23:59:35","No","No","No","Internal","valve to renew at next opportunity. As it is  a black out job"]
[null,null,null,10857,null,"45_20/03/2020 12:25:38 PM","2020-03-04T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","FWG ejector pump's suction pipe flange is salt soaked. To renew gasket and cleaned.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related,Knowledge Based","10.29","Medium","","","Gasket renewed , no leaks ","2020-03-22T23:59:35","","Completed","2020-03-13T23:59:35","No","No","No","Internal"]
[null,null,null,10858,null,"45_20/03/2020 12:44:50 PM","2020-03-04T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","DG FO supply pump no 2 to overhaul, leaking from seal.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Pump  overhauled, mechanical seal and bearing renewed.No leaks","2020-03-28T23:59:35","","Completed","2020-03-29T23:59:35","No","No","No","Internal"]
[null,null,null,10859,null,"45_20/03/2020 4:00:44 PM","2020-03-04T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","On deck various chains are in rusted condition. To derust and paint.","Deck - Pipe / Fittings","General Appearance","External Factors","6.2","High","","","de rusted & painetd","2020-04-25T23:59:35","","Completed","2020-04-21T23:59:35","No","No","No","Internal"]
[null,null,null,10860,null,"45_20/03/2020 4:02:42 PM","2020-03-04T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Area below U-bolt to derust and paint in loaded passage.","Deck - Pipe / Fittings","General Appearance","External Factors,Human Error","6.2","High","","","to derust & paint","2021-03-07T23:59:35","","Completed","2021-03-06T23:59:35","No","No","No","Internal","Job is in progress, Target date revised."]
[null,null,null,10861,null,"45_20/03/2020 4:08:03 PM","2020-03-04T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Midship store natural vent cover to clean and paint.","Deck - Pipe / Fittings","General Appearance","External Factors,Human Error","6.2","High","","","Cleaned.","2020-03-18T23:59:35","","Completed","2020-03-15T23:59:35","No","No","No","Internal"]
[null,null,null,10862,null,"45_20/03/2020 4:09:34 PM","2020-03-04T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Steam line main valve for slop tank on deck to paint, as same is in rusty condition.","Deck - Pipe / Fittings","General Appearance","External Factors,Human Error","6.2","High","","","de rusted & painted","2020-04-26T23:59:35","","Completed","2020-03-04T23:59:35","No","No","No","Internal"]
[null,null,null,10863,null,"45_20/03/2020 12:36:09 PM","2020-03-04T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","MGPS anode is just lying on floor. Proper securing arrangement to make","Miscellaneous","Eng. / Strg. Comp.","Behaviour Based,Human Error","10.29","Medium","","","MGPS anode shifted and secured in designated stand.","2020-03-21T23:59:35","","Completed","2020-03-11T23:59:35","No","No","No","Internal"]
[null,null,null,10864,null,"45_20/03/2020 12:09:11 PM","2020-03-04T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Frosting noted i nmeat room fish room.Manual defrosting by hot water to be carried out twice a month.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related,Knowledge Based","10.29","Medium","","","Manual defrosting have been done and same will be followed twice a month.","2020-03-19T23:59:35","","Completed","2020-03-09T23:59:35","No","No","No","Internal"]
[null,null,null,10865,null,"45_20/03/2020 12:39:27 PM","2020-03-04T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","No.2 ME canshaft L.O booster pump suction pressure gauge to renew. Even with Main L.O pump stopped, it is showing pressure.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related,Human Error,Knowledge Based","10.29","Medium","","","Pressure gauge renewed.","2020-03-19T23:59:35","","Completed","2020-03-11T23:59:35","No","No","No","Internal"]
[null,null,null,10866,null,"45_20/03/2020 4:05:38 PM","2020-03-04T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Forward store hatch cover to paint.","Deck - Pipe / Fittings","General Appearance","External Factors,Human Error","6.2","High","","","Derusted, 3 coats primer applied & painted.","2020-03-21T23:59:35","","Completed","2020-03-12T23:59:35","No","No","No","Internal"]
[null,null,null,10867,null,"45_20/03/2020 4:13:10 PM","2020-03-04T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Meat room, Fish room, veg room to arrange in better manner.","Accommodation","General Appearance","External Factors","6.2","High","","","Vessel received provisions for 2 months & almost all racks are full. All empty cartons removed & arranged the racks as practicable as possible.","2020-04-10T23:59:35","","Completed","2020-03-12T23:59:35","No","No","No","Internal"]
[null,null,null,11572,null,"45_30/04/2020 6:50:00 AM","2020-03-22T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Platform holding bolts of cranes to be renewed","Deck - Machinery","Structural Condn. / WT integrity ","External Factors","11.6","Medium","","","Based on the condition of the removed bolts, it is not required to renew the bolts. (Mail rcvd from suptd. on 18 May 2020).","2020-06-22T23:59:35","","Completed","2020-05-10T23:59:35","No","No","No","Internal"]
[null,null,null,11348,null,"45_07/04/2020 8:35:20 PM","2020-03-26T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Aux. Boiler # 2 exhaust pipe expansion joint found with crack.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Expansion joint to be replaced. RO raised.               Refman job created","2020-09-22T23:59:35","SCAN 200094","Completed","2020-07-22T23:59:35","Yes","No","No","Internal","Job Assigned to DD"]
[null,null,null,13518,null,"45_16/08/2020 9:10:30 AM","2020-03-27T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","ME LO pump breaker no.2 found heated up and on inspection Y phase of breaker found black","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","On inspection it was found that cradle spring was loose and this caused into overheating of the cradle as well. Upon receiving new cradle along with MCCB same was replaced by isolating the bus tie breaker for GSP no.2","2020-08-06T23:59:35","","Completed","2020-07-29T23:59:35","No","No","No","Internal"]
[null,null,null,11574,null,"45_01/05/2020 8:23:50 AM","2020-03-28T23:59:35","Defect","Ship Staff","Ship Staff Insp.","LT cooler (100% ) sea water inlet pipe line leaking at bend due to  material wastage/hole","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","The pipeline bend at the sea water outlet of LT cooler renewed with pre fabricated bend recieved from shore.","2020-04-12T23:59:35","","Completed","2020-04-09T23:59:35","No","No","No","Internal"]
[null,null,null,11575,null,"45_01/05/2020 8:30:28 AM","2020-03-29T23:59:35","Defect","Ship Staff","Suptd. Insp.","Atm. condenser Sea water oulet pipe bend found leaking due to material wastage /hole","Deck - Pipe / Fittings","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Sea water oulet piupe bend renewed with prefabricated bend received from shore workshop","2020-04-22T23:59:35","","Completed","2020-04-09T23:59:35","No","No","No","Internal"]
[null,null,null,11349,null,"45_07/04/2020 12:46:20 PM","2020-03-29T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Foundation bolts of AFT ETA sheared off whilst testing. 2 bolts were drilled off & re instated with new ones","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","External Factors","","","","","All bolts renewed","2020-06-28T23:59:35","","Completed","2020-06-06T23:59:35","No","No","No","Internal"]
[null,null,null,11467,null,"45_17/04/2020 8:33:14 AM","2020-04-05T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Auxiliary  Boiler#2 atomizing steam valve found leaking","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Valve replaced with spare, no leaks.","2020-04-07T23:59:35","","Completed","2020-04-06T23:59:35","No","No","No","Internal"]
[null,null,null,11573,null,"45_01/05/2020 8:10:56 AM","2020-04-07T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Fressh water generator#1 jacket water inlet/outlet butterfly valves are stuck and not able to operate with handle.","E/R - Aux. Mach.,E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Renewed both jacket water  inlet& outlet valve of FWG#1. ","2020-06-22T23:59:35","","Completed","2020-06-14T23:59:35","No","No","No","Internal"]
[null,null,null,12022,null,"45_02/06/2020 8:32:49 AM","2020-04-23T23:59:35","Observation","Ship Staff","Ship Staff Insp.","W.O INCINERATOR FURNACE REFRACTORY FOUND DAMAGED AT SOME AREA.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","REFRACTORY REPAIRED.","2020-05-07T23:59:35","","Completed","2020-04-30T23:59:35","No","No","No","Internal"]
[null,null,null,12023,null,"45_02/06/2020 8:44:50 AM","2020-05-02T23:59:35","Observation","Ship Staff","Ship Staff Insp.","COPT L.O COOLER #2 AND #2  S.W PRESSURE GAUGE FOUND FAULTY","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","PRESSURE GAUGE RENEWED","2020-05-22T23:59:35","","Completed","2020-05-06T23:59:35","No","No","No","Internal"]
[null,null,null,11919,null,"45_19/05/2020 3:14:16 AM","2020-05-03T23:59:35","Defect","Ship Staff","Ship Staff Insp.","ME unit #6 crankcase door found leaking ","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Crankcase door gasket renewed.","2020-05-07T23:59:35","","Completed","2020-05-05T23:59:35","No","No","No","Internal"]
[null,null,null,12019,null,"45_02/06/2020 9:22:23 AM","2020-05-04T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Chief engineer's office ship viewer computer not working.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Trouble shooting has been carried out as per office instructions, still found not working. CPU to be renewed.","2020-09-22T23:59:35","","Completed","2020-10-16T23:59:35","No","No","No","Internal"]
[null,null,null,11918,null,"45_19/05/2020 2:55:13 AM","2020-05-12T23:59:35","Defect","Ship Staff","Ship Staff Insp.","AE flow meter not working ","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Flowmeter renewed, found working satisfactory","2020-08-22T23:59:35","SCAN200105","Completed","2020-07-07T23:59:35","No","No","No","Internal"]
[null,null,null,12024,null,"45_02/06/2020 8:38:37 AM","2020-05-16T23:59:35","Defect","Ship Staff","Ship Staff Insp.","VACUUME TOILET LINE FOUND CHOCKE MAKING VACUUME TOILET SYSTEM IN OPERATIONAL.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","PIPE SECTIONS REMOVED AND PIPE CLEARED AND FITTED BACK. SYSTEM WORKING NORMAL.","2020-05-17T23:59:35","","Completed","2020-05-16T23:59:35","No","No","No","Internal"]
[null,null,null,12020,null,"45_02/06/2020 9:33:08 AM","2020-05-20T23:59:35","Defect","Ship Staff","Ship Staff Insp.","VECS O2% INDICATION NOT SHOWING CORRECTLY AND NONFLOW ALARM NOT WORKING.","Inert Gas","Cargo / Ballast Systems","Equipment Related","8.17","Low","","","VECS conrol box including O2 sensor renewed. System functioning normally.","2020-09-22T23:59:35","SCAN200112","Completed","2020-09-30T23:59:35","No","No","No","Internal"]
[null,null,null,12021,null,"45_01/06/2020 11:43:52 PM","2020-05-20T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Pressure lines / Return lines of winches (W1, W2, W3, W5 & W8) have thinned down &  W3 return line having pin hole.","Deck - Mooring Machinery","Mooring","External Factors,Human Error","","","","","All thinned downed & temporary repaired lines renewd at Yiu Lian ship yard","2020-09-22T23:59:35","","Completed","2020-11-01T23:59:35","No","No","No","Internal"]
[null,null,null,12770,null,"45_18/06/2020 2:40:13 AM","2020-06-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Emergency switch board - bus tie breaker UVT controller defective","Elect. Mach. & Equip.","Emgcy. Systems","Equipment Related","10.37","Medium","","","UVT renewed","2020-09-22T23:59:35","","Completed","2020-06-30T23:59:35","No","No","No","Internal"]
[null,null,null,12997,null,"45_01/07/2020 9:36:22 AM","2020-06-15T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","CCTV to be installed at various places - CCR, ECR, Eng Room, Bridge facing deck area.","Miscellaneous","Communication","Equipment Related","","","","","Equipments recieved, intallation preparation work to be done by ship staff.Installation to be done by shore technician","2020-09-22T23:59:35","","Completed","2020-09-11T23:59:35","No","No","No","Internal"]
[null,null,null,12998,null,"45_01/07/2020 2:23:37 AM","2020-06-22T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Port Provision crane minor oil leakage  observed from luffing cylinder seal","Deck - Machinery","General Appearance","Equipment Related","8.76","Medium","","","Luffing cylinder seal to be renewed. Job included in REFMAN","2020-09-22T23:59:35","SCAN200115","Completed","2020-07-23T23:59:35","No","No","No","Internal"]
[null,null,null,13519,null,"45_16/08/2020 9:26:01 AM","2020-06-29T23:59:35","Defect","Ship Staff","Ship Staff Insp.","MOS panel on MSBD found not working","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","Upon inspection TFT of MOS panel found faulty. Same was replaced with spare MOS panel and setup/commisioning done according to procedure given in manual.","2020-08-06T23:59:35","","Completed","2020-08-04T23:59:35","No","No","No","Internal"]
[null,null,null,13199,null,"45_18/07/2020 4:59:51 AM","2020-07-07T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","#1 A/E Fuel oil booster pump, found vibrating and leaking from seal, On opening up, found oil in armature of the motor.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Replaced with spare new motor, and pump replaced with spare overhauled pump. Tried out found satisfactory","2020-07-08T23:59:35","","Completed","2020-07-07T23:59:35","No","No","No","Internal"]
[null,null,null,13520,null,"45_16/08/2020 9:20:37 AM","2020-07-07T23:59:35","Defect","Ship Staff","Ship Staff Insp.","ME Aux blower no.1 motor not getting started in Auto","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","On troubleshooting it was found on delay timer H3BAN was malfunctioning. Same was replaced during stoppage of ME and tried out.","2020-07-23T23:59:35","","Completed","2020-07-17T23:59:35","No","No","No","Internal"]
[null,null,null,13295,null,"45_31/07/2020 9:16:22 AM","2020-07-09T23:59:35","Defect,Observation","Ship Staff","Ship Staff Insp.","During previous  discharge,moderate Steam leakage from bonet gasket of steam dumping valve was noticed.","E/R - Pipes/ valves & fittings","Cargo / Ballast Systems","Equipment Related","10.32","Very High","","","1. Drains before valve found shut, same opened to drain condensate from lines, and practice maintained, to keep drain open at sea, to avoid, damage of gasket due to hammering.                2.System depressurised, and bonet gasket renewed","2020-07-10T23:59:35","","Completed","2020-07-10T23:59:35","No","No","No","Internal"]
[null,null,null,13299,null,"45_31/07/2020 9:53:58 AM","2020-07-09T23:59:35","Defect,Observation","Ship Staff","Ship Staff Insp.","Vacuum pump found cutting in 4 times in 1 minute.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Vacuum toilet eductor opened up for inspection,found one bolt on flap loose, hence flap not sitting in place, and therefore loss of vacuum, same rectified,cleaned, and fit back, now working satisfactory.","2020-07-17T23:59:35","","Completed","2020-07-15T23:59:35","No","No","No","Internal"]
[null,null,null,13300,null,"45_31/07/2020 9:33:49 AM","2020-07-11T23:59:35","Breakdown,Defect,Observation","Ship Staff","Ship Staff Insp.","1. M.D.O Starboard manifold valve found seized .                                                               2.Dresser coupling on M.D.O line bolts found excessivelly rusted.                                          3. M.D.O storage tank valve found hard.","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","Equipment Related","6.7","High","","","1. Gear box of valve opened up, found gear broked, renewed valve with new spare.                       2.Dresser coupling bolts, replaced with new bolts.   3.Gear case, of M.D.O storage tank valve opened up, and found excessive rust, same cleaned, filled with new grease,and new gasket, eased up.","2020-07-11T23:59:35","","Completed","2020-07-12T23:59:35","No","No","No","Internal"]
[null,null,null,13296,null,"45_31/07/2020 10:06:22 AM","2020-07-12T23:59:35","Breakdown,Defect","Ship Staff","Ship Staff Insp.","VRCS pump found not developing pressure, and hydraullic valves not operating from remote position","Cargo Mach.,Deck - Machinery,Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","10.32","Very High","","","1. Found relief valve in open condition,and short cycling of oil taking place, same overhaulled.         2. unloader solenoid, actuating the relief valve, found without  supply, on investigating, found pcb of unloader valve, burnt, same rectified by soldering.now working satisfactory ","2020-07-12T23:59:35","","Completed","2020-07-12T23:59:35","No","No","No","Internal"]
[null,null,null,13297,null,"45_31/07/2020 9:00:59 AM","2020-07-15T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","After discharging, vessel at low draught, deck Seal low flow alram sounded, followed by low level alarm.Deck seal Pump casings found excessively hot and developing low   pressure of 2.3 bar .Pumps changed over and found no improvement.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","1. Since the  fault being common,  pipe sections opened up and checked for blockages  but found clear.                                                                      2. Both Deck Seal pumps opened up for inspection, and clarances measured, found to be satisfactory. Vanes found blocked with shells, and dirt, same cleaned with chemical ,Both pumps tried out, found working satisfactory, Both pumps developing 4.5 bar pressure.      ","2020-07-16T23:59:35","","Completed","2020-07-16T23:59:35","No","No","No","Internal"]
[null,null,null,13298,null,"45_31/07/2020 8:31:19 AM","2020-07-20T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","1.Found fuel rack stuck and engine found excessively speeding                                                               2.L.o condition/colour in the sump found deteorated/discoloured.                             ","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.27","Medium","","","1.Fuel pump overhauled, ,found , control sleeve teeth broken, same turned 180 deg .                       2.Relay HB36D1 found in poor condition ( stop solenoid)  same renewed.                                       3 L.o in both lifeboat engines renewed","2020-07-20T23:59:35","","Completed","2020-07-20T23:59:35","No","No","No","Internal"]
[null,null,null,13294,null,"45_01/08/2020 8:22:17 AM","2020-07-23T23:59:35","Other","Ship Staff","Ship Staff Insp.","Sewage overbaoard  discharge rate chart for DHT Scandinavia  is not endorsed by class","E/R - Aux. Mach.","Eng. / Strg. Comp.","Industry Issue","10.32","Very High","","","Endorsed copy pasted on sewage holding tank","2020-08-23T23:59:35","","Completed","2020-07-30T23:59:35","No","No","No","Internal","Endorsed copy has already been sent  to vessel."]
[null,null,null,13521,null,"45_16/08/2020 9:38:27 AM","2020-07-26T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","AC motor no.2 found making abnormal sound and vibration","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","AC compressor no.2 was found in stand still condition from long time and on changing over,it was found running proper for a week but after that it was found that abnormal sound and vibration is coming from NDE of motor. So it was stopped and changed over to no.1. Upon inspection/opening it was found that brinelling was there on motor bearings as it was in standstill condition for long time with tension on driving belts. So motor was overahuled and AC compressor oil renwal and routines. Same was tried out and found running smooth. ","2020-08-06T23:59:35","","Completed","2020-08-02T23:59:35","No","No","No","Internal"]
[null,null,null,13522,null,"45_16/08/2020 2:26:28 AM","2020-07-27T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","Bilge pump tried out and found mechanical seal leaking excessively.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Pump opened up for inspection, and renewed line bearing and mechanical seal.","2020-07-29T23:59:35","","Completed","2020-07-27T23:59:35","No","No","No","Internal"]
[null,null,null,13523,null,"45_16/08/2020 2:36:52 AM","2020-07-28T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","a)1 pc pipe bender found defective.                            b)2 pcs vacuum bucket found disfuntioning","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","a)Teflon, seals and piston fabricated, now working satisfactory. Now being used to fabricate/bend pipes.                                                         b) O-ring /seals renewed, now working satisfactory,being used in e/r for maintainance purpose.","2020-07-28T23:59:35","","Completed","2020-07-28T23:59:35","No","No","No","Internal"]
[null,null,null,13532,null,"45_16/08/2020 3:01:36 AM","2020-07-29T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","a)vacuum tiolet found chocked by using face tissue paper.                                                            b)pipes internal diameter, found reduced due to excessive deposit in pipes.                                   c)loss of vacuum in the system","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related,External Factors,Human Error,Inappropriate Procedure","10.32","Very High","","","a) various sections in e/r opened up, cleared.          b) 4 sections cleared with high pressure gun, before being fit back.                                             c) vacuum leakage found in upper deck toilet, leakage rectified.","2020-07-29T23:59:35","","Completed","2020-07-29T23:59:35","No","No","No","Internal"]
[null,null,null,13524,null,"45_16/08/2020 4:35:35 AM","2020-07-30T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","Hydraulic leak on deck during sts operation from mooring winch return line.","Deck - Mooring Machinery,Deck - Pipe / Fittings","Eng. / Strg. Comp.","Equipment Related","","","","","leak temporarily arrested, sinse vessel in port.New pipe fabricated , and fitted back after completion of 1st loading.","2020-07-30T23:59:35","","Completed","2020-08-01T23:59:35","No","No","No","Internal"]
[null,null,null,13525,null,"45_16/08/2020 4:45:13 AM","2020-07-30T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","# 1 HFO purifeed pump leaking from  mechanical seal after a couple of days of running.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Seal renewed,and put into use, working satisfactory","2020-07-31T23:59:35","","Completed","2020-07-31T23:59:35","No","No","No","Internal"]
[null,null,null,13526,null,"45_16/08/2020 6:26:07 AM","2020-08-01T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","a)# 1 fwg , found not building up sufficient vacuuum.                                                                    b)Short cyling of fresh water, through high salinity solenoid valve when shut.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","a)#1 fwg  eductor opened up for inspection, found holed at throat, bronze putty applied.            b) additional ball cock fitted in line and kept shut.","2020-08-04T23:59:35","","Completed","2020-08-04T23:59:35","No","No","No","Internal"]
[null,null,null,13527,null,"45_16/08/2020 5:00:04 AM","2020-08-02T23:59:35","Defect,Observation","Ship Staff","Ship Staff Insp.","Boiler water circulating pump #2 outlet valve found leaking from bonet gasket.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Depressurised and drained entire line, gasket renewed for both pump  discharge valves.","2020-08-03T23:59:35","","Completed","2020-08-03T23:59:35","No","No","No","Internal"]
[null,null,null,13528,null,"45_16/08/2020 6:54:07 AM","2020-08-02T23:59:35","Breakdown,Defect","Ship Staff","Ship Staff Insp.","a)Found drop in pressure on Lp side of main air compressor # 2 .                                                   b)Lp side relief valve found lifting                              c) Lp liner found scratching marks, dents. Piston crown top found dented .                              d)  Crankase l.o discoloured","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Opened up compressor, found lp side suction valve plate broken,same renewed with new spare, and lapped delivery valve plate and fitted.     b)Relief valve on Lp side renewed with new spare.                                                                                c) Lp liner opened up, straches smoothed lightly, with rough stone. piston rings found intact.                      d)L.O renewed and sump cleaned,                ","2020-08-05T23:59:35","","Completed","2020-08-05T23:59:35","No","No","No","Internal"]
[null,null,null,13529,null,"45_16/08/2020 9:55:00 AM","2020-08-03T23:59:35","Breakdown,Defect","Ship Staff","Ship Staff Insp.","AE FO circulating motor no.1 found making abnormal sound and vibration ","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","On changing over to stand by motors it was found making abnormal sound and vibration. Upon dismantelling the motor NDE bearing casing of motor was found loose and bearing was damage. Same was repaired and motor was overhauled. Tried out after installation and was found running properly.","2020-08-12T23:59:35","","Completed","2020-08-03T23:59:35","No","No","No","Internal"]
[null,null,null,13530,null,"45_16/08/2020 7:33:38 AM","2020-08-04T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","During routine check/firing of incinerator, found primary burner not firing.","E/R - Aux. Mach.,Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","primary burnerattached  pump opened up for inspection found                                                                                 a) valve seized  same eased up                                             b)  Filter fully chocked, same cleaned.  Now working satisfactory                                                           ","2020-08-06T23:59:35","","Completed","2020-08-06T23:59:35","No","No","No","Internal"]
[null,null,null,13531,null,"45_16/08/2020 7:02:55 AM","2020-08-05T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","When trying to chemical clean main air coolers, found 90 % of nozzles blocked on both air coolers","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Both Air cooler pipes, on which nozzles are fitted, removed from air coolers, nozzles cleared, and put back, gaskets renewed","2020-08-07T23:59:35","","Completed","2020-08-07T23:59:35","No","No","No","Internal"]
[null,null,null,13533,null,"45_16/08/2020 7:22:29 AM","2020-08-05T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","During routine maintanance ,was unable to isolate the A/E Backwash filter, suspecting  a)backwashing drain valve not holding, and oil from the mixing column head continiously  flowing back to the filter.                               b)change over  block mechanism o-ring leaking","E/R - Pipes/ valves & fittings,Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","a) System drained, and new valve fitted.                          b)Change over block found seized and was unable to pull out, same jacked, o-ring renewed, and fitted back.","2020-08-05T23:59:35","","Completed","2020-08-05T23:59:35","No","No","No","Internal"]
[null,null,null,13914,null,"45_04/09/2020 6:39:26 AM","2020-08-13T23:59:35","Breakdown,Defect","Ship Staff","Ship Staff Insp.","2  Sections of the Winch hydraullic return line found leaking","Deck - Mooring Machinery,Deck - Pipe / Fittings","Mooring","Equipment Related","","","","","2 New hydraullic line sectiones fabricated in workshop and fitted on deck","2020-08-15T23:59:35","","Completed","2020-08-14T23:59:35","No","No","No","Internal"]
[null,null,null,13915,null,"45_04/09/2020 7:01:37 AM","2020-08-14T23:59:35","Breakdown,Defect","Ship Staff","Ship Staff Insp.","a).# 1 HFO purifier found Excessive vibration during discharging.                                                                 b).Bowl found overflowing.","E/R - Purifier","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Purifier opened up for inspection , found bowl nut  loose. Major overhaul carried out, bearings renewed , O-rings renewed , Clearances , height checked, Axial Vibration checked, found to be satisfactory. Purifier boxed back and tried out, found satisfactory","2020-08-19T23:59:35","","Completed","2020-08-17T23:59:35","No","No","No","Internal"]
[null,null,null,13916,null,"45_04/09/2020 7:07:16 AM","2020-08-15T23:59:35","Breakdown,Observation","Ship Staff","Ship Staff Insp.","UV sterilizer found not functioning, uv sterilizer filter found  dirty.                          Mineralizer dolomite filter dirty,                                 ","E/R - Aux. Engine,Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","UV sterilizer made operational. Dolomite granules cleaned, UV filter renewed. ","2020-08-15T23:59:35","","Completed","2020-08-15T23:59:35","No","No","No","Internal"]
[null,null,null,13917,null,"45_05/09/2020 9:24:30 AM","2020-08-17T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","#2 HFO purifier, found overflowing, and excessive vibration while discharging. Also found excessive vibration from motor non drive end bearing","E/R - Purifier","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","a)Purifier opened up, bowl cleaned, new o-ring and seal ring fitted.                                                                    b)Non drive end bearing casing found worn out,new bearings fitted with shim insert in non drive end.                                                                            .c) Friction pads renewed.                                               .Purifier boxed back and tried out, found working satisfactory.                                                              ","2020-08-19T23:59:35","","Completed","2020-08-19T23:59:35","No","No","No","Internal"]
[null,null,null,16130,null,"45_27/09/2020 11:11:02 AM","2020-08-30T23:59:35","Defect","Ship Staff","Ship Staff Insp.","No.1 boiler water level SIPART controller found malfunctioning and was not able to cope up with the water required by boiler.This resulted in alarm and tripping of boiler.","E/R - Boiler,Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","SIPART controller YWAY value, SCDUR value found was not proper, same was changed and initilisation of SIPART carried out and upperstream band as well as lower stream band adjusted before initialisation. After initialisation it was tried out and found working satisfactory.","2020-09-07T23:59:35","","Completed","2020-09-03T23:59:35","No","No","No","Internal"]
[null,null,null,16131,null,"45_03/10/2020 2:04:49 PM","2020-09-10T23:59:35","Defect,Observation","Ship Staff","Ship Staff Insp.","# 1 economiser feed pump found not coping up,when running at anchorage","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","# 1 economiser feed pump overhaulled, with new bearing, mouth ring, mechanical seals, sleeve, o-ring ,gaskets and put into use, now running satisfactory while running at anchorage.","2020-09-14T23:59:35","","Completed","2020-09-14T23:59:35","No","No","No","Internal"]
[null,null,null,16132,null,"45_03/10/2020 1:55:02 PM","2020-09-11T23:59:35","Defect","Ship Staff","Engineering Audit","#1 M/E fo circulating pump found leaking from mechanical seal/abnormal vibration sounded when started same.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","previously overhauled,M/E  f.o circulating pump which was kept ready to use state , put into use, and found out that overhaulled  pump also leaking from the seal, both pumps overhauled with new bearings and seals. one put into use, now running satisfactory","2020-09-11T23:59:35","","Completed","2020-09-11T23:59:35","No","No","No","Internal"]
[null,null,null,16133,null,"45_27/09/2020 10:58:56 AM","2020-09-12T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","NO.1 IG Blower Main breaker at 440V feeder panel of MSBD found malfunctioning due to failure of holding coil. ","Cargo Mach.,Elect. Mach. & Equip.","Cargo / Ballast Systems","Equipment Related","10.32","Very High","","","Old breaker HiBL 403 NE removed and new breaker UPB 400H installed having same capacity of 400Amps and and shunt trip coil of 220V.","2020-09-22T23:59:35","","Completed","2020-09-16T23:59:35","No","No","No","Internal"]
[null,null,null,16134,null,"45_03/10/2020 2:21:17 PM","2020-09-21T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","# 2 FWG ejector pump found leaking from the seal ","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","#2 fwg ejector pump, overhaulled  with new bearings,mechanical seals, mouth rings and casing ring, sleeve and o-rings ","2020-09-22T23:59:35","","Completed","2020-09-22T23:59:35","No","No","No","Internal"]
[null,null,null,16805,null,"45_05/01/2021 11:48:27 AM","2020-10-14T23:59:35","Defect,Observation","Ship Staff","Ship Staff Insp.","#3 A/E ,oil consumption too high, and external jacket  water leakage from #5  head ","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","#3 A/E , # 1 unit  piston opened up for inspection , found piston rings butt  clearances inline.renewed piston rings . and # 5 head leakage rectified by renewing o-rings","2020-12-23T23:59:35","","Completed","2020-12-15T23:59:35","No","No","No","Internal"]
[null,null,null,16135,null,"45_17/12/2020 7:23:59 PM","2020-10-22T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Portable Fire extinquisher, from steering flat removed from place during DD due to installation of EGCS effluent water outlet panel ","LSA / FFA","Eng. / Strg. Comp.","Equipment Related","5.33","High","","","Fire extinquisher fitted back with new modified bracket","2020-12-22T23:59:35","","Completed","2020-11-04T23:59:35","No","No","No","Internal"]
[null,null,null,16136,null,"45_16/12/2020 2:13:58 PM","2020-10-25T23:59:35","Observation","Ship Staff","Ship Staff Insp.","EEBD removed from location during DD due to installation of VFD pumps","LSA / FFA","Eng. / Strg. Comp.","Equipment Related","5.44","High","","","EEBD Kept back in place with new braket fitted","2020-11-07T23:59:35","","Completed","2020-11-05T23:59:35","No","No","No","Internal"]
[null,null,null,16124,null,"45_18/11/2020 11:18:52 PM","2020-10-27T23:59:35","Defect,Observation","Ship Staff","Ship Staff Insp.","SAAB tank RADAR gauging system - SCD touch function found defective","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.12","Medium","","","Service engineer attended the vessel on 4th feb 2021. Rectified the problem.","2021-02-11T23:59:35","","Completed","2021-01-27T23:59:35","No","No","No","Internal"]
[null,null,null,16137,null,"45_16/12/2020 1:45:12 PM","2020-10-28T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Portable foam extinquisher on boiler platform found lashed with rope, and locking pin bracket damaged","LSA / FFA","Eng. / Strg. Comp.","Equipment Related","5.33","High","","","Locking pin bracket repaired","2020-12-07T23:59:35","","Completed","2020-11-29T23:59:35","No","No","No","Internal"]
[null,null,null,16144,null,"45_18/11/2020 11:23:27 PM","2020-11-04T23:59:35","Observation","Ship Staff","Ship Staff Insp.","WBT gauging system - Levelmaster - H8 communication failure alarm triggers frequently","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.12","Medium","","","As per service technician report, H8 utility software will be required to identify defect.","2020-11-13T23:59:35","","Completed","2020-11-12T23:59:35","No","No","No","Internal"]
[null,null,null,16806,null,"45_05/01/2021 12:28:43 PM","2020-11-06T23:59:35","Observation","Ship Staff","Ship Staff Insp.","17 different types of stem , water, f.o leaks in engine room originated after DD and found few defective pressure gauges/thermometers","E/R - Aux. Engine,E/R - Aux. Mach.,E/R - Boiler,E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","All leaks nipped up, by isolating various systems.    various pressure gauges in engine replaced with new spare.","2020-12-23T23:59:35","","Completed","2020-12-20T23:59:35","No","No","No","Internal"]
[null,null,null,16145,null,"45_08/12/2020 5:04:09 PM","2020-11-10T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Fire hydrant next to 2C leaking","Critical Equip.","Safety / LSA / FFA","Equipment Related","","","","","Hydrant valve leak rectified.","2020-12-07T23:59:35","","Completed","2020-11-21T23:59:35","No","No","No","Internal"]
[null,null,null,16128,null,"45_14/12/2020 11:30:37 AM","2020-11-11T23:59:35","Defect,Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Gap between pipe and deck house bulkhead, same on M/E and D/G  exhaust pipe penetration from Engine casing","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","Staging  erected and job completed","2021-01-23T23:59:35","","Completed","2021-01-17T23:59:35","No","No","No","Internal","Job to be planned in ballast voyage. Target date revised. Presently vessel in discharge port."]
[null,null,null,16138,null,"45_16/12/2020 1:53:10 PM","2020-11-11T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Ship Staff Insp.","Reserve Fuel oil level in emergency generator tank found below minimum mark","Critical Equip.,LSA / FFA","Eng. / Strg. Comp.","Equipment Related","10.35","Very High","","","Reserve fuel tank topped up to minimum mark to run for 18 hrs on full load condition in accordance with solas","2020-12-12T23:59:35","","Completed","2020-11-14T23:59:35","No","No","No","Internal"]
[null,null,null,16139,null,"45_08/12/2020 1:36:22 PM","2020-11-11T23:59:35","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Accommodation panel to clean off hand stain.","Accommodation","General Appearance","Behaviour Based","11.1","High","","","All panels of accommodation cleaned with soap and water.","2020-11-13T23:59:35","","Completed","2020-11-12T23:59:35","No","No","No","Internal"]
[null,null,null,16140,null,"45_08/12/2020 1:42:03 PM","2020-11-11T23:59:35","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Suez canal crew room bed curtain hanging loose","Accommodation","General Appearance","Behaviour Based","11.1","High","","","suez canal crew room bed curtain fixed.","2020-11-13T23:59:35","","Completed","2020-11-13T23:59:35","No","No","No","Internal"]
[null,null,null,16141,null,"45_08/12/2020 1:59:35 PM","2020-11-11T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Suez canal cabin weather tight door packing channel to chip and paint.","Accommodation","General Appearance","Inappropriate Procedure","11.17","Low","","","Suez canal cabin weather tight door packing channel chipped and painted.","2020-11-17T23:59:35","","Completed","2020-11-16T23:59:35","No","No","No","Internal"]
[null,null,null,16142,null,"45_08/12/2020 2:14:56 PM","2020-11-11T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Slop tank (P) steam pipe deck penetration pieces to derust and paint. ","Deck - Pipe / Fittings","Cargo / Ballast Systems","External Factors","8.5","Very High","","","Slop tank (P) steam pipe deck penetration pieces derusted and painted. ","2020-11-15T23:59:35","","Completed","2020-11-14T23:59:35","No","No","No","Internal"]
[null,null,null,16143,null,"45_08/12/2020 4:12:05 PM","2020-11-11T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","COT 4P dry check port cap holding wire broken.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Human Error","8.12","Medium","","","COT 4P dry check port cap holding wire renwed.","2020-11-22T23:59:35","","Completed","2020-11-14T23:59:35","No","No","No","Internal"]
[null,null,null,16146,null,"45_08/12/2020 4:28:03 PM","2020-11-11T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Helicopter safety toolbox-suggested keep equipment list in the box for cross check .","Critical Equip.","Cargo / Ballast Systems","Human Error","2.3","High","","","Helicopter safety toolbox equipment list kept in the box .","2020-11-17T23:59:35","","Completed","2020-11-14T23:59:35","No","No","No","Internal"]
[null,null,null,16147,null,"45_08/12/2020 4:36:00 PM","2020-11-11T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Mid ship store (P) ventilation duck at FWD froze.","Hull & Tanks","Cargo / Ballast Systems","Human Error","11.6","Medium","","","FWD  ventilation duck of Mid ship store (P) freed , greased, descaled and painted.","2020-12-07T23:59:35","","Completed","2020-11-27T23:59:35","No","No","No","Internal"]
[null,null,null,16148,null,"45_08/12/2020 4:41:58 PM","2020-11-11T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","COT 3P COW line under side rust spots to derust and paint.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Human Error","11.5","Medium","","","COT 3P COW line under side rust spots derusted and painted","2020-12-07T23:59:35","","Completed","2020-11-29T23:59:35","No","No","No","Internal"]
[null,null,null,16149,null,"45_08/12/2020 4:46:36 PM","2020-11-11T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Hydraulic valve box no.2 cover holding wing nuts missing.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Human Error","11.5","Medium","","","Hydraulic valve box no.2 cover holding fitted with new wing nuts.","2020-12-06T23:59:35","","Completed","2020-11-25T23:59:35","No","No","No","Internal"]
[null,null,null,16150,null,"45_08/12/2020 4:52:18 PM","2020-11-11T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Hydraulic valve box no.2 hyd oil inlet valve hand wheel broken.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","11.5","Medium","","","Hydraulic valve box no.2 hyd oil inlet valve hand wheel fitted.","2020-12-04T23:59:35","","Completed","2020-11-24T23:59:35","No","No","No","Internal"]
[null,null,null,16151,null,"45_08/12/2020 4:58:10 PM","2020-11-11T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Main deck cable next to no.2 COT(C) manhole hanging loose-to secure with cable ties to secure with adequate cable tie.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Human Error","11.5","Medium","","","Main deck cable next to no.2 COT(C) manhole tied and securired with adequate cable tie.","2020-11-25T23:59:35","","Completed","2020-11-20T23:59:35","No","No","No","Internal"]
[null,null,null,16152,null,"45_08/12/2020 5:10:31 PM","2020-11-11T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","All mooring winche oil case cap frozen and oil glass opaque.","Deck - Mooring Machinery","Mooring","Equipment Related","9.14","Medium","","","All mooring winche oil case cap freed greased and oil sight glass cleaned.","2020-12-06T23:59:35","","Completed","2020-11-26T23:59:35","No","No","No","Internal"]
[null,null,null,16153,null,"45_08/12/2020 5:14:23 PM","2020-11-11T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Bosun store davit SWL to paint with contrast (black) colour.","Deck - Machinery","General Appearance","Human Error","8.63","High","","","Bosun store davit SWL to painted with contrast (black) colour.","2020-12-08T23:59:35","","Completed","2020-11-25T23:59:35","No","No","No","Internal"]
[null,null,null,16154,null,"45_08/12/2020 5:20:04 PM","2020-11-11T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","F'cle deck dead man roller to SWL to paint with contrast colour(White).","Deck - Mooring Machinery","Mooring","Human Error","9.19","Low","","","F'cle deck dead man roller to SWL painted with contrast colour(White).","2020-12-07T23:59:35","","Completed","2020-11-27T23:59:35","No","No","No","Internal"]
[null,null,null,16155,null,"45_08/12/2020 4:19:22 PM","2020-11-11T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","FO bunker manifold (P) FWD pressure guage showing 3.5 bars although bunker recived from STBD side. Pls check whether valve is leaking or pressure guage is defective and take necessary action.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Human Error","6.7","High","","","The pipe fitted to the pressure guage found choked same cleaned and fitted back.","2020-11-17T23:59:35","","Completed","2020-11-13T23:59:35","No","No","No","Internal"]
[null,null,null,16156,null,"45_08/12/2020 5:26:51 PM","2020-11-11T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Bosun store local fire-fighting system start panel blocked.","Critical Equip.","Safety / LSA / FFA","Human Error","5.4","High","","","Bosun store local fire-fighting system start panel block cleared.","2020-11-18T23:59:35","","Completed","2020-11-13T23:59:35","No","No","No","Internal"]
[null,null,null,16157,null,"45_08/12/2020 6:02:34 PM","2020-11-11T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Life buoys kept in bosun stores.","LSA / FFA","Safety / LSA / FFA","Human Error","5.31","High","","","Life buoys kept in their respective places.","2020-11-13T23:59:35","","Completed","2020-11-12T23:59:35","No","No","No","Internal"]
[null,null,null,16158,null,"45_08/12/2020 6:06:43 PM","2020-11-11T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","One spare valve lying near mast riser -to shift to mid ship store.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Human Error","5.11","Low","","","One spare valve lying near mast riser shifted to mid ship store.","2020-11-23T23:59:35","","Completed","2020-11-18T23:59:35","No","No","No","Internal"]
[null,null,null,16159,null,"45_08/12/2020 6:13:09 PM","2020-11-11T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Pump room housekeeping to improve.Metal scraps, chain etc lying on tank top.","Cargo Mach.","Cargo / Ballast Systems","Human Error","8.51","Low","","","Pump room cleaned and removed Metal scraps, chain etc lying on tank top .","2020-12-02T23:59:35","","Completed","2020-11-30T23:59:35","No","No","No","Internal"]
[null,null,null,16160,null,"45_08/12/2020 6:20:10 PM","2020-11-11T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Mooring winch M12 platform lip wasted.","Deck - Mooring Machinery","Mooring","External Factors","9.14","Medium","","","Mooring winch M12 platform lip damage cleared.","2020-12-07T23:59:35","","Completed","2020-11-29T23:59:35","No","No","No","Internal"]
[null,null,null,16161,null,"45_08/12/2020 6:23:49 PM","2020-11-11T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Gymnasium untidy","Accommodation","General Appearance","Human Error","11.1","High","","","Gymnasium cleaned and arranged.","2020-12-05T23:59:35","","Completed","2020-11-25T23:59:35","No","No","No","Internal"]
[null,null,null,16162,null,"45_08/12/2020 6:29:28 PM","2020-11-11T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Pump room EEBD box cover brocken.","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.27","Medium","","","Pump room EEBD box cover fixed.","2020-12-05T23:59:35","","Completed","2020-11-26T23:59:35","No","No","No","Internal"]
[null,null,null,16163,null,"45_09-Dec-20 1:45:08 AM","2020-11-11T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Notice board pen holder filled with trash.","Accommodation","General Appearance","Behaviour Based","11.1","High","","","Removed trash from notice board pen holder. ","2020-11-14T23:59:35","","Completed","2020-11-12T23:59:35","No","No","No","Internal"]
[null,null,null,16164,null,"45_09-Dec-20 1:48:19 AM","2020-11-11T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Deck above paint lock to derust and paint.","Accommodation","General Appearance","External Factors","11.1","High","","","Derusted and painted on deck above paint locker. ","2020-12-07T23:59:35","","Completed","2020-11-30T23:59:35","No","No","No","Internal"]
[null,null,null,16165,null,"45_09-Dec-20 1:56:33 AM","2020-11-11T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","EGCS deck house fire extinguishers to be included in firefighting equipment booklet and also tag for monthly condition check to attach.","LSA / FFA","Safety / LSA / FFA","Human Error","5.27","Medium","","","EGCS deck house fire extinguishers included in firefighting equipment booklet and also taged for monthly condition and attached.","2020-11-18T23:59:35","","Completed","2020-11-14T23:59:35","No","No","No","Internal"]
[null,null,null,16166,null,"45_09-Dec-20 2:00:12 AM","2020-11-11T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Engine casing at aft stained - to clean and paint.","Accommodation","General Appearance","External Factors","11.1","High","","","Engine casing at aft cleaned and painted.","2020-12-07T23:59:35","","Completed","2020-11-29T23:59:35","No","No","No","Internal"]
[null,null,null,16167,null,"45_09-Dec-20 2:05:31 AM","2020-11-11T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Cable tray joining bracket missing at few laocations.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Human Error","11.5","Medium","","","Cable tray joining bracket fixed back.","2020-11-29T23:59:35","","Completed","2020-11-19T23:59:35","No","No","No","Internal"]
[null,null,null,16168,null,"45_09-Dec-20 1:51:42 AM","2020-11-11T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","FO tank save all tray (next to pump room entrance P) plug missing.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Human Error","8.12","Medium","","","FO tank save all tray (next to pump room entrance P) pluged.","2020-11-15T23:59:35","","Completed","2020-11-13T23:59:35","No","No","No","Internal"]
[null,null,null,16169,null,"45_12/12/2020 1:10:09 PM","2020-11-11T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Loose slings on top of BWTS filters in pump room to secure.","Cargo Mach.","Cargo / Ballast Systems","Human Error","5.11","Low","","","Loose slings on top of BWTS filters in pump room secured","2020-11-14T23:59:35","","Completed","2020-11-13T23:59:35","No","No","No","Internal"]
[null,null,null,16170,null,"45_20/12/2020 10:22:21 AM","2020-11-11T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","LT cooler gaskets stowed in box . Its likelythat gaskets will be permanently deformed at the bend and crack.","E/R - Pipes/ valves & fittings,Miscellaneous","Eng. / Strg. Comp.","Equipment Related,Inappropriate Procedure","10.32","Very High","","","New stand fabricated for stowing gaskets , to prevent from twisting of gaskets","2020-11-22T23:59:35","SCAN200112","Completed","2020-11-17T23:59:35","No","No","No","Internal"]
[null,null,null,16171,null,"45_20/12/2020 10:44:48 AM","2020-11-11T23:59:35","Defect,Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Bulkhead insulation covering aft of  D/G#2 exhaust uptake to repair","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Human Error","10.32","Very High","","","New insulation fitted at aft portion of D/G # 2 uxhaust uptake","2020-12-22T23:59:35","","Completed","2020-11-18T23:59:35","No","No","No","Internal"]
[null,null,null,16172,null,"45_20/12/2020 10:52:39 AM","2020-11-11T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Boiler water circulating pump pressure gauges hanging loose","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Boiler water circulating pump and other pumps pressure gauges  secured","2020-11-22T23:59:35","","Completed","2020-11-13T23:59:35","No","No","No","Internal"]
[null,null,null,16173,null,"45_20/12/2020 11:11:28 AM","2020-11-11T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Ship Staff Insp.","#5 Aft fuel injector return line pipe slight leakage from union","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.19","Very High","","","Union tightened and leak rectified","2020-11-13T23:59:35","","Completed","2020-11-12T23:59:35","No","No","No","Internal"]
[null,null,null,16174,null,"45_11/12/2020 10:22:38 PM","2020-11-11T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Main deck cable tray support bracket rusted ,to derust and paint.","Deck - Pipe / Fittings","Cargo / Ballast Systems","External Factors","11.5","Medium","","","Main deck cable tray support bracket derusted and painted.","2020-12-04T23:59:35","","Completed","2020-11-20T23:59:35","No","No","No","Internal"]
[null,null,null,16175,null,"45_20/12/2020 1:06:51 PM","2020-11-11T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Scavenge air cooler (aft) cooling water outlet valve handle missing","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","New handle fitted","2020-12-11T23:59:35","","Completed","2020-11-14T23:59:35","No","No","No","Internal"]
[null,null,null,16176,null,"45_20/12/2020 1:17:30 PM","2020-11-11T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Sewage plant tray to derust & paint","Miscellaneous","General Appearance","External Factors","10.32","Very High","","","Sewage plant tray painting carried out.","2020-12-11T23:59:35","","Completed","2020-11-14T23:59:35","No","No","No","Internal"]
[null,null,null,16177,null,"45_20/12/2020 1:22:04 PM","2020-11-11T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ODME Oil content meter air leakage","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","6.13","Low","","","Pipe fittings renewed","2020-12-12T23:59:35","","Completed","2020-11-14T23:59:35","No","No","No","Internal"]
[null,null,null,16178,null,"45_20/12/2020 1:02:15 PM","2020-11-11T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","M/E T/C (aft) manometer water level not visible","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Manometer filled with water.","2020-12-07T23:59:35","","Completed","2020-11-14T23:59:35","No","No","No","Internal"]
[null,null,null,16179,null,"45_20/12/2020 1:29:39 PM","2020-11-11T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","LO drain filter vent valve hand wheel missing","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","New handwheel fitted","2020-11-20T23:59:35","","Completed","2020-11-14T23:59:35","No","No","No","Internal"]
[null,null,null,16180,null,"45_20/12/2020 1:36:36 PM","2020-11-11T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Stern tube oil tank level less then normal mark","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Oil topped up.","2020-11-22T23:59:35","","Completed","2020-11-14T23:59:35","No","No","No","Internal"]
[null,null,null,16181,null,"45_20/12/2020 1:32:57 PM","2020-11-11T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Scavenge air cooler drain pipe sight glass dirty.","E/R - Main Engine","General Appearance","Equipment Related","10.32","Very High","","","Sight glass cleaned.","2020-11-22T23:59:35","","Completed","2020-11-14T23:59:35","No","No","No","Internal"]
[null,null,null,16182,null,"45_20/12/2020 1:39:06 PM","2020-11-11T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Engine room tank top aft of flywheel area to clean","Miscellaneous","General Appearance","External Factors","10.29","Medium","","","Area cleaned of oil and water","2020-11-22T23:59:35","","Completed","2020-11-14T23:59:35","No","No","No","Internal"]
[null,null,null,16183,null,"45_20/12/2020 1:41:40 PM","2020-11-11T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ME unit 3 cam space covered with oil","E/R - Main Engine","General Appearance","Equipment Related","10.19","Very High","","","Camspace space cleaned and source of leak rectified.","2020-11-14T23:59:35","","Completed","2020-11-14T23:59:35","No","No","No","Internal"]
[null,null,null,16190,null,"45_20/12/2020 1:45:26 PM","2020-11-11T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Metal scraps lying in the funnel space.","Miscellaneous","General Appearance","Human Error","10.29","Medium","","","Metal scrap removed and area cleaned","2020-11-22T23:59:35","","Completed","2020-11-14T23:59:35","No","No","No","Internal"]
[null,null,null,16125,null,"45_11/12/2020 10:17:21 PM","2020-11-11T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Various Pipes on main deck have rust spots.pipe to derust to chip.","Deck - Pipe / Fittings","Cargo / Ballast Systems","External Factors","8.3","Very High","","","To derust and paint","2021-03-08T23:59:35","","Completed","2021-03-05T23:59:35","No","No","No","Internal","Job in progress. Target date revised."]
[null,null,null,16126,null,"45_11/12/2020 10:25:44 PM","2020-11-11T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Few deck pipe U clamp rusted , to renew.","Deck - Pipe / Fittings","Cargo / Ballast Systems","External Factors","8.3","Very High","","","Renew rusted U clamps.","2021-02-08T23:59:35","","Completed","2021-01-04T23:59:35","No","No","No","Internal","Job in progress. Target date revised."]
[null,null,null,16127,null,"45_11/12/2020 10:30:11 PM","2020-11-11T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Main deck spot rusts to derust and paint.","Hull & Tanks","Cargo / Ballast Systems","External Factors","11.1","High","","","Spot derusting & painting of main deck area completed.","2021-04-22T23:59:35","","Completed","2021-03-31T23:59:35","No","No","No","Internal","Job is progress. Target date revised."]
[null,null,null,16184,null,"45_17/12/2020 7:44:18 PM","2020-11-20T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Main engine # 6 cylinder lubricator found scoring marks on plungers when previously opend up in DD by servive engineer.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Same renewed with new spare received and lubrication checked, found to be satisfactory","2020-11-30T23:59:35","","Completed","2020-11-21T23:59:35","No","No","No","Internal"]
[null,null,null,16185,null,"45_16/12/2020 2:20:44 PM","2020-11-23T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Both main air compressors 1 and 2, stud found broken on LP and HP side respectively","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Both compressor, cylinder heads removed. broken studs, drilled and removed using stud extractor.","2020-11-25T23:59:35","","Completed","2020-11-24T23:59:35","No","No","No","Internal"]
[null,null,null,16186,null,"45_17/12/2020 7:35:53 PM","2020-11-23T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Oil leaking from seal of turning gear","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Gear wheel removed from place and new oil seal renewed.","2020-11-25T23:59:35","","Completed","2020-11-24T23:59:35","No","No","No","Internal"]
[null,null,null,16189,null,"45_16/12/2020 2:27:42 PM","2020-11-24T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","#2 Hfo Purifier found slightly vibrating","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","#2 Hfo purifier opened up for inspection, bowl cleaned, found, bown nut loose, same cleaned and bowl nut tightened @ 100 n-m ","2020-11-27T23:59:35","","Completed","2020-11-26T23:59:35","No","No","No","Internal"]
[null,null,null,16187,null,"45_17/12/2020 7:14:31 PM","2020-11-27T23:59:35","Defect,Observation","Ship Staff","Ship Staff Insp.","Galley overboard pipe section before overboardvalve found holed, and water leaking into engine room","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","New pipe fabricated and fitted back","2020-11-29T23:59:35","","Completed","2020-11-29T23:59:35","No","No","No","Internal"]
[null,null,null,16188,null,"45_07/12/2020 7:37:20 PM","2020-11-28T23:59:35","Breakdown,Observation","Ship Staff","Ship Staff Insp.","Upper deck common toilet flush non functional.Toilet kept untidy .","Accommodation","MLC Related","Equipment Related","11.13","Low","","","On troubleshooting found that control valve and water valve malfunctioning. Same repaired and fitted back. Working satisfactorily.Toilet cleaned ","2020-12-17T23:59:35","","Completed","2020-11-29T23:59:35","No","No","No","Internal"]
[null,null,null,11340,null,"45_30/03/2020 3:38:19 PM","2020-12-02T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Gangways Operating area need to be Guarded.","Deck - Pipe / Fittings","General Appearance","External Factors,Human Error","6.2","High","","","Need to get Guard fabricated onboard ship's workshop.","2021-01-22T23:59:35","","Completed","2021-01-06T23:59:35","Yes","No","No","Internal"]
[null,null,null,16807,null,"45_05/01/2021 1:06:03 PM","2020-12-07T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Ingress of condensate water found in Engine room service air line.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Aux boiler no.2 atomising air valve found leaking,non return check valve spring found damaged,same replaced with sapre.Ball valve seal and packing replaced with new spare","2020-12-23T23:59:35","","Completed","2020-12-22T23:59:35","No","No","No","Internal"]
[null,null,null,11347,null,"45_07/04/2020 8:29:13 PM","2020-12-11T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Inventory management: All spare parts to be checked, varified and update in PAL with correct storing location.","Documentation","ISM Related","Equipment Related","10.12","Very High","","","All spare parts to be checked, varified and update in PAL with correct storing location.Job in progress","2021-03-17T23:59:35","","Completed","2021-03-17T23:59:35","No","No","No","Internal"]
[null,null,null,16808,null,"45_05/01/2021 2:36:06 PM","2020-12-15T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","UV Sterilizer giving abnormal alarm","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","On inspection it was found ballast was burnt and not working and UV light glass found broken. Same was renewed and new ballast installed from pump room light. Since these are not being used as we have converted it into LEDs","2021-01-23T23:59:35","","Completed","2020-12-16T23:59:35","No","No","No","Internal"]
[null,null,null,16809,null,"45_03/01/2021 11:34:43 AM","2020-12-19T23:59:35","Defect","Ship Staff","Ship Staff Insp.","#1 fwg ejector pump found leaking from the seal","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","# 1 FWG Pump opened up for inspection and seal renewed.anodes found completly wasted and pump casing corroded,same rectified by cold repair.Pump motor overhauled both ends bearings replaced with new spare.","2020-12-23T23:59:35","","Completed","2020-12-22T23:59:35","No","No","No","Internal"]
[null,null,null,17713,null,"45_25/01/2021 9:43:06 AM","2020-12-27T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","#1 Main air compressor, coupling found broken ","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Motor removed from place, renewed new gear and coupling. Tried out, now running satisfactory.","2020-12-28T23:59:35","","Completed","2020-12-27T23:59:35","No","No","No","Internal"]
[null,null,null,17714,null,"45_25/01/2021 11:25:48 AM","2020-12-28T23:59:35","Observation","Ship Staff","Ship Staff Insp.","#1 Refregeration compressor overhauling record not found. Mechanical seal found leaking","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Refregeration compressor overhauled with new spares, piston , con rod and mechanical seal renewed. tried out found satisfactory","2021-01-08T23:59:35","","Completed","2021-01-07T23:59:35","No","No","No","Internal"]
[null,null,null,16804,null,"45_05/01/2021 2:25:19 PM","2021-01-06T23:59:35","Breakdown,Critical Equipment","Ship Staff","Ship Staff Insp.","OWS found not starting.On inspection it was found PLC is showing error 6401.It means it is having sum check error.","Critical Equip.","MARPOL Related","Equipment Related","","","",""," RO 215009 raised for service attendance. Technician attended the vessel on 4 FEB 21, renewed the PLC with new spare, set the timer values. Found the system working satisfactory.","2021-01-23T23:59:35","","Completed","2021-01-27T23:59:35","No","No","No","Internal"]
[null,null,null,17712,null,"45_25/01/2021 8:47:21 PM","2021-01-07T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Salinometer found malfunctioning at cascade tank","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","salinometer changed with new spare.","2021-05-07T23:59:35","","Completed","2021-04-03T23:59:35","No","No","No","Internal"]
[null,null,null,17715,null,"45_25/01/2021 11:32:22 AM","2021-01-07T23:59:35","Breakdown,Defect","Ship Staff","Ship Staff Insp."," Inert gas  high temperature  sensor  found corroded, leading to tripping of IG plant","Inert Gas","Eng. / Strg. Comp.","Equipment Related","8.3","Very High","","","Spare IG sensor fitted, now working satisfactory","2021-02-07T23:59:35","","Completed","2021-01-17T23:59:35","No","No","No","Internal"]
[null,null,null,17716,null,"45_25/01/2021 7:49:30 PM","2021-01-14T23:59:35","Breakdown,Defect","Ship Staff","Ship Staff Insp.","#1 main air compressor, 2 LP side studs found broken","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","All four studs on LP Side renewed with new studs","2021-01-15T23:59:35","","Completed","2021-01-14T23:59:35","No","No","No","Internal"]
[null,null,null,18205,null,"45_03/03/2021 3:43:54 PM","2021-01-27T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Paint peel of @ several places on main deck","Hull & Tanks","General Appearance","External Factors","11.1","High","","","All loose paint removed on main deck from Midship to Accomodation block & Re-painted with 2 coats of primer followed by top coat.","2021-04-25T23:59:35","","Completed","2021-04-24T23:59:35","No","No","No","Internal"]
[null,null,null,18206,null,"45_09/03/2021 11:52:56 PM","2021-01-27T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Aft FWG evaporator plates leaking.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Evaporatot side gaskets renewed with sapre new gasket and leakage rectified.","2021-04-22T23:59:35","SCAN210044","Completed","2021-04-02T23:59:35","No","No","No","Internal"]
[null,null,null,18207,null,"45_13/03/2021 5:06:07 PM","2021-01-27T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","EGCS RECORD BOOK NOT MAINTAINED","Documentation","MARPOL Related","Equipment Related","10.11","Medium","","","EGCS PARAMETES READINGS ARE RECORDED IN ENGINE ROOM LOG BOOK AND FULL PARAMETER READINGS ARE DOWLOADED  FROM EGCS PANEL AND RECORDED SEPARATELY IN COMPUTER. AWATING FOR EGCS RECORD BOOK. ","2021-04-22T23:59:35","","Completed","2021-03-16T23:59:35","No","No","No","Internal"]
[null,null,null,18208,null,"45_03/03/2021 3:54:03 PM","2021-01-27T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Windlass brake adjustment – match marking not there.","Deck - Mooring Machinery","Mooring","Equipment Related","9.14","Medium","","","Windlass brake adjustment – match marking.","2021-02-27T23:59:35","","Completed","2021-02-26T23:59:35","No","No","No","Internal"]
[null,null,null,18209,null,"45_09/03/2021 11:43:13 PM","2021-01-27T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ME lube oil purifier operated at 71 degree celsius inlet temperature","E/R - Purifier","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","ME lube oil purifier operating temperature adjusted to 92 degree celsius.","2021-02-06T23:59:35","","Completed","2021-01-28T23:59:35","No","No","No","Internal"]
[null,null,null,18210,null,"45_09/03/2021 11:45:39 PM","2021-01-27T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","All cargo pumps bulkhead seal grease level low.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.45","High","","","All cargo pumps bulkhead seal grease topped up full.","2021-02-06T23:59:35","","Completed","2021-02-02T23:59:35","No","No","No","Internal"]
[null,null,null,18211,null,"45_09/03/2021 11:48:21 PM","2021-01-27T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Steam leak from no:-1 HFO purifier temp control valve.","E/R - Purifier","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Temp control valve spindle bush tightened and steam leakage rectified.","2021-02-24T23:59:35","","Completed","2021-01-31T23:59:35","No","No","No","Internal"]
[null,null,null,18212,null,"45_10/03/2021 12:01:11 AM","2021-01-27T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ME LO auto back wash filter aft chamber rotation is slow","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","ME LO auto back wash filter driving hydraulic motor overhauled, found wear and tear in driving slots, defective spare changed and tried out, found in good order.","2021-03-27T23:59:35","","Completed","2021-02-25T23:59:35","No","No","No","Internal"]
[null,null,null,18213,null,"45_10/03/2021 12:10:19 AM","2021-01-27T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","EGCS room need cleaning","Miscellaneous","General Appearance","Equipment Related","10.29","Medium","","","EGCS room cleaning completed.","2021-02-24T23:59:35","","Completed","2021-02-16T23:59:35","No","No","No","Internal"]
[null,null,null,18214,null,"45_10/03/2021 12:18:38 AM","2021-01-27T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Lamp fused in emergency escape","Elect. Mach. & Equip.","Safety / LSA / FFA","Equipment Related","10.15","Low","","","Lamp changed with spare lamp.","2021-02-01T23:59:35","","Completed","2021-01-27T23:59:35","No","No","No","Internal"]
[null,null,null,18215,null,"45_03/03/2021 3:36:44 PM","2021-01-27T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","IG pipe section near deck seal vent has signs of leakage.","Deck - Pipe / Fittings","General Appearance","External Factors","8.23","Medium","","","No leaks found.","2021-03-12T23:59:35","","Completed","2021-03-05T23:59:35","No","No","No","Internal"]
[null,null,null,18216,null,"45_10/03/2021 12:05:45 AM","2021-01-27T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Oil sheen in aft bilge well","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Aft bilge well cleaning to be carriedout.","2021-03-27T23:59:35","","Completed","2021-02-24T23:59:35","No","No","No","Internal"]
[null,null,null,18087,null,"45_01/03/2021 7:27:45 PM","2021-02-20T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Required new plate gaskets for no.1 fresh water generator.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Defective gaskets renewed with new gasket.","2021-03-24T23:59:35","SCAN210044","Completed","2021-04-02T23:59:35","No","No","No","Internal"]
[null,null,null,18460,null,"45_31/03/2021 9:35:31 PM","2021-03-17T23:59:35","Defect","Ship Staff","Ship Staff Insp.","starboard grey water line in engine room bottom platform found leaking from seam.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","permanent repair carried out by renewing the pipe.","2021-04-22T23:59:35","","Completed","2021-03-29T23:59:35","No","No","No","Internal"]
[null,null,null,18459,null,"45_31/03/2021 9:23:39 PM","2021-03-23T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","Fwd piston horn found not  working, same opened for inspection, piston and connecting rod broken in to small peices and liner got damaged due to broken connecting rod and piston","Navigation - Others","Communication","Equipment Related","12.12","High","","","All damaged parts renewed and tried out.","2021-05-23T23:59:35","","Completed","2021-03-24T23:59:35","No","No","No","Internal"]
[null,null,null,9594,null,"45_12/01/2020 9:55:38 AM","2021-03-26T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Aux boiler no:-2 aux feed water line auto control valve gland seal is leaking.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Auto control valve gland seal renew with new gland seal kit and leakage rectified.","2021-04-17T23:59:35","","Completed","2021-04-06T23:59:35","No","No","No","Internal","Job in progress, Target date revised accordingly."]
[null,null,null,18979,null,"45_30/04/2021 2:38:01 PM","2021-04-01T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","M14 mooring winch, operating control unit hydralic pipe line uniion connection found leaking.","Deck - Pipe / Fittings","Mooring","Equipment Related","9.14","Medium","","","Defective union connections renewed and leakage rectified.","2021-05-22T23:59:35","","Completed","2021-04-23T23:59:35","No","No","No","Internal"]
[null,null,null,18980,null,"45_30/04/2021 2:43:39 PM","2021-04-01T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Windlass stbd hydraulic block pipe connection leaking.","Deck - Machinery","Mooring","Equipment Related","9.14","Medium","","","O-ring renewed for the flange connections and leakage rectified.","2021-05-22T23:59:35","","Completed","2021-04-25T23:59:35","No","No","No","Internal"]
[null,null,null,19500,null,"45_03/05/2021 20:00:30","2021-04-01T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Insulation matt in front of electrical panels in bosun store missing","Miscellaneous","General Appearance","Behaviour Based","10.24","Low","","","Insulation matt placed in front of electrical panel in bosun store.","2021-04-16T23:59:35","","Completed","2021-04-07T23:59:35","No","No","No","Internal"]
[null,null,null,19501,null,"45_03/05/2021 20:19:29","2021-04-01T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Air Con compressor no. 2 suction & discharge pressure gauge defective","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","External Factors","10.32","Very High","","","Defective gauge replaced with new spare.","2021-04-30T23:59:35","","Completed","2021-04-10T23:59:35","No","No","No","Internal"]
[null,null,null,19502,null,"45_03/05/2021 20:21:31","2021-04-01T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","LT cooler no 1 & 2 SW inlet flange slight leakage / covered with salt\n\n","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","External Factors","10.31","Very High","","","Flange disconnected, gasket renewed and leakage rectified..","2021-05-31T23:59:35","","Completed","2021-04-22T23:59:35","No","No","No","Internal"]
[null,null,null,19503,null,"45_03/05/2021 20:24:16","2021-04-01T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Rubber matt in front of EGCS remote I/O cabinet missing","E/R - Pumps","General Appearance","Behaviour Based,Human Error","10.24","Low","","","Rubber mat placed in front of EGCS remote cabinet.","2021-05-15T23:59:35","","Completed","2021-04-11T23:59:35","No","No","No","Internal"]
[null,null,null,19504,null,"45_03/05/2021 20:26:16","2021-04-01T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","440V feeder circuit resistance less than infinity","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Behaviour Based,Human Error","10.38","Medium","","","No:-1 engine room vent fan junction box contain little moisture inside it. So box opened up and made it as water tight and 440v resistance reached infinity.","2021-04-08T23:59:35","","Completed","2021-04-07T23:59:35","No","No","No","Internal"]
[null,null,null,19505,null,"45_03/05/2021 20:27:50","2021-04-01T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Emergency Generator 220V feeder circuit resistance less than infinity","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Behaviour Based,Human Error","10.38","Medium","","","Light casing outside the Paint locker contain little moisture inside it, casing renewed and resistance increased to infinity.","2021-04-08T23:59:35","","Completed","2021-04-04T23:59:35","No","No","No","Internal"]
[null,null,null,19506,null,"45_03/05/2021 19:45:20","2021-04-01T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Accommodation front wall to spot de-rust & paint","Miscellaneous","General Appearance","External Factors","11.8","Low","","","Accomodation front wall Cleaned, Spot Derusted & Re-Painted","2021-06-30T23:59:35","","Completed","2021-04-23T23:59:35","No","No","No","Internal"]
[null,null,null,19507,null,"45_03/05/2021 19:56:00","2021-04-01T23:59:35","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Gym equipment to secure","Accommodation","General Appearance","External Factors","11.13","Low","","","Gym Equipment secured with Anti-Skid mats","2021-04-30T23:59:35","","Completed","2021-04-23T23:59:35","No","No","No","Internal"]
[null,null,null,19508,null,"45_03/05/2021 19:58:06","2021-04-01T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Paint drum over stacked, provide additional securing arrangement\n\n","Miscellaneous","General Appearance","Behaviour Based,Human Error","9.14","Medium","","","Additional securing arrangement fabricated & put in place; Paints are now safely stacked/ stored.","2021-04-30T23:59:35","","Completed","2021-04-24T23:59:35","No","No","No","Internal"]
[null,null,null,19509,null,"45_03/05/2021 19:49:12","2021-04-01T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Weather deck on top of Pump room to derust & paint","Miscellaneous","General Appearance","External Factors","11.8","Low","","","Weather deck on top of pumproom Derusting - Buffing followed by 2 coat Primer & Final top coat completed.","2021-04-30T23:59:35","","Completed","2021-04-28T23:59:35","No","No","No","Internal"]
[null,null,null,19510,null,"45_03/05/2021 20:31:07","2021-04-01T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Include SOX scrubber deck house smoke detectors in monthly report\n\n\n\n","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Inappropriate Procedure","5.35","Medium","","","SOX scrubber deck house Smoke detectors included in Monthly Report","2021-04-15T23:59:35","","Completed","2021-04-04T23:59:35","No","No","No","Internal"]
[null,null,null,19511,null,"45_03/05/2021 20:02:35","2021-04-01T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Main Deck electric cable support wasted at STBD side of value box 1A","Deck - Pipe / Fittings","General Appearance","External Factors","11.5","Medium","","","Main Deck electric cable support renewed & put back in place.","2021-04-30T23:59:35","","Completed","2021-04-30T23:59:35","No","No","No","Internal"]
[null,null,null,18982,null,"45_15/04/2021 7:17:01 PM","2021-04-06T23:59:35","Defect","Ship Staff","Ship Staff Insp.","AFT ETA storage box cabinet door hinges are broken.","Deck - Mooring Machinery,Miscellaneous","General Appearance","Equipment Related,External Factors","11.3","Medium","","","AFT ETA storage box cabinet door hinges renewed.","2021-04-12T23:59:35","","Completed","2021-04-10T23:59:35","No","No","No","Internal"]
[null,null,null,18981,null,"45_15/04/2021 7:49:52 PM","2021-04-07T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Port side Pumproom blower not Operational due to broken coupling in motor side.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","5.18","High","","","pump room coupling fabricated onboard and assembled in motor and tried out, currently it is working fine. intermediate coupling inspection carried out .Requisition raised, original spare received onboard and kept as spare.","2021-07-06T23:59:35","SCAN210081","Completed","2021-06-10T23:59:35","No","No","No","Internal"]
[null,null,null,19497,null,"45_14/05/2021 3:42:16 PM","2021-04-24T23:59:35","Defect","Ship Staff","Ship Staff Insp.","VALVE REMOTE CONTROL SYSTEM PUMP OUTLET PRESSURE GAUGE FAULTY","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Pressure gauge renewed with new pressure gauge","2021-06-22T23:59:35","SCAN210094","Completed","2021-06-02T23:59:35","No","No","No","Internal"]
[null,null,null,19496,null,"45_03/05/2021 19:28:32","2021-04-25T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Paint peel of on main deck at various isolated locations from midship to Foc'scle.","Miscellaneous","General Appearance","External Factors","11.1","High","","","Derusting/ Scrapping followed by 2 coats of primer & Spot Final Coat completed on Port Side main deck Fwd to midship.","2021-07-25T23:59:35","","Completed","2021-06-08T23:59:35","No","No","No","Internal"]
[null,null,null,19726,null,"45_15/06/2021 12:32:19 PM","2021-04-27T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Repeater panel MN400 on the bridge giving EXT alarm E1 WBT system fault.","Elect. Mach. & Equip.","Cargo / Ballast Systems","Equipment Related","10.32","Very High","","","Checked the system, repeater panel is common for both pump room gas alarm system and water ballast tank system. theres is no alarm in th main panel in CCR, all checks carried out as per technician advice. seems to be configuration error. Issue Rectified by shore technician @ Singapore 17 Aug 2021","2021-08-23T23:59:35","SCAN 215045","Completed","2021-08-09T23:59:35","No","No","No","Internal","Service engineer will be arranged inSingapore."]
[null,null,null,19498,null,"45_14/05/2021 9:21:25 PM","2021-04-28T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Maine engine unit no6 fuel pump leakage.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","changed with spare overhauled fuel pump","2021-07-23T23:59:35","","Completed","2021-06-22T23:59:35","No","No","No","Internal"]
[null,null,null,19499,null,"45_14/05/2021 11:27:17","2021-05-06T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Unable to start/ Run both WBP simultaneously for De-ballasting operation using BWTS system ","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","6.21","High","","","Defect Added in GC list.","2021-08-05T23:59:35","","Completed","2021-05-24T23:59:35","No","No","No","Internal"]
[null,null,null,19545,null,"45_31/05/2021 9:14:20 PM","2021-05-06T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Main engine fuel leak off alarm sensor malfunctioning. ","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Replaced with new spare.","2021-08-23T23:59:35","scan210074","Completed","2021-06-01T23:59:35","No","No","No","Internal"]
[null,null,null,19540,null,"45_30/05/2021 9:48:47 PM","2021-05-09T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","Fwd piston horn found not  working, same opened for inspection, piston and connecting rod in broken condition.","Navigation - Others","Communication","Equipment Related","12.12","High","","","overhauled with new spare.","2021-08-23T23:59:35","SCAN210075","Completed","2021-06-02T23:59:35","No","No","No","Internal"]
[null,null,null,19541,null,"45_30/05/2021 9:52:35 PM","2021-05-10T23:59:35","Defect","Ship Staff","Ship Staff Insp.","HYDROPHORE PUMP DISCHARGE NON RETURN VALVE DISC NOT CLOSING PROPERLY.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","New valve replaced.","2021-08-22T23:59:35","SCAN210095","Completed","2021-06-04T23:59:35","No","No","No","Internal"]
[null,null,null,19539,null,"45_28/05/2021 16:08:32","2021-05-12T23:59:35","Defect","Ship Staff","Ship Staff Insp.","During Routine Inspection of FPK WBT vent head, found vent float is broken.","Deck - Pipe / Fittings,Hull & Tanks","Structural Condn. / WT integrity ","Equipment Related","11.7","High","","","Renewed with new float.","2021-08-11T23:59:35","SCAN210100","Completed","2021-06-07T23:59:35","No","No","No","Internal"]
[null,null,null,19542,null,"45_30/05/2021 10:00:03 PM","2021-05-14T23:59:35","Defect","Ship Staff","Ship Staff Insp.","AFT PEAK TANK FCV3211 VALVE MALFUNCTIONING, NEED TECHNICIAN ASSISTANCE OR TO RENEW THE VALVE UNDER GURANTEE CLAIM","Miscellaneous","Cargo / Ballast Systems","Equipment Related","","","","","TECHNICIAN came onboared and rectified the faults.","2021-08-21T23:59:35","","Completed","2021-05-30T23:59:35","No","No","No","Internal"]
[null,null,null,19543,null,"45_30/05/2021 9:55:41 PM","2021-05-15T23:59:35","Defect","Ship Staff","Ship Staff Insp.","HFO PURIFIER CLEAN OIL OUTLET FLEXIBLE HOSE LEAKING.","E/R - Purifier","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","fexible hose renewed with new spare.","2021-09-22T23:59:35","SCAN210104","Completed","2021-08-27T23:59:35","No","No","No","Internal","Spares on order, will bee supplied once ready."]
[null,null,null,19544,null,"45_28/05/2021 16:16:29","2021-05-16T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Ballast tank level gauging - Level master H8   is giving frequent alarm/ Error; \"“BLOCKERR” LED illuminated","Miscellaneous","Cargo / Ballast Systems","Equipment Related","8.13","Medium","","","H8 Utility software CD installed and tried out, alarms start indicating in panel, still the problem persists. Rectified by Shore Technician @ Singapore on 17 Aug 2021.","2021-08-15T23:59:35","SCAN 215047","Completed","2021-08-09T23:59:35","No","No","No","Internal","send mail with present status."]
[null,null,null,19991,null,"45_18/06/2021 14:13:34","2021-05-30T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Fwd of manifold – main deck coating at various stages of paint peel off","Miscellaneous","General Appearance","External Factors","11.1","High","","","Derusting/ Buffing followed by 2 coat of primer & Spot Final coat painting completed.","2021-08-29T23:59:35","","Completed","2021-08-08T23:59:35","No","No","No","Internal","Please update progress on same with every DDRL."]
[null,null,null,19992,null,"45_27/6/2021 9:53:57 AM","2021-05-30T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Personal transfer basket - More than 7 years old – to raise RO for replacement","Miscellaneous","Safety / LSA / FFA","Inappropriate Procedure","5.47","Medium","","","New Personal Transfer Basket Procured & put in use,Old Personal transfer basket discarded from Use. Received new personal transfer basket @ Singapore 17 Aug 2021.","2021-08-29T23:59:35","SCAN 210118","Completed","2021-08-09T23:59:35","No","No","No","Internal","Spare on order, will be supplied at next call Singapore."]
[null,null,null,19993,null,"45_29/06/2021 12:20:12 AM","2021-05-30T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Fish room and meat room door handles broken – to procure new handle and replace","Miscellaneous","General Appearance","Equipment Related","11.17","Low","","","New hanlde changed.","2021-08-22T23:59:35","SCAN210127","Completed","2021-08-13T23:59:35","No","No","No","Internal"]
[null,null,null,19994,null,"45_18/06/2021 13:30:27","2021-05-30T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Ship Staff Insp.","Rudder angle indicator shows an error of 3 degree from local Auto pilot panel","Navigation - Others","Navigation","Equipment Related","10.41","Medium","","","Required to adjust from steering gear room informed to kamlesh solanki regarding this issue. Torque motor, control rod lever turn buckle adjusted. It was working fine for few days. Again the problem raised. will do the fine tuning and will update in next report.","2021-08-23T23:59:35","","Completed","2021-07-30T23:59:35","No","No","No","Internal","Target date revised, as need to adjust again."]
[null,null,null,19995,null,"45_18/06/2021 13:27:20","2021-05-30T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","EGCS tower room\tNatural vent wire mesh in various stages of corrosion","Miscellaneous","General Appearance","External Factors","11.7","High","","","EGCS tower room -\tNatural vent wire mesh & Flap Derusted followed by 1 Coat primer & Final coat Completed.","2021-06-18T23:59:35","","Completed","2021-06-18T23:59:35","No","No","No","Internal"]
[null,null,null,19996,null,"45_18/06/2021 14:11:13","2021-05-30T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Fire wire reel Seized and not turning – greasing points painted over","Deck - Mooring Machinery","Mooring","Behaviour Based,Human Error","9.14","Medium","","","Fwd & Aft Fire wire reel freed up, Grease nipples renewed & Lubricated.","2021-06-24T23:59:35","","Completed","2021-06-11T23:59:35","No","No","No","Internal"]
[null,null,null,19997,null,"45_29/06/2021 12:23:35 AM","2021-05-30T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Damper near Top up air compressor – seized, not able to operate by remote leverOn ","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","damper removed from duct, derusted, eased up, painted, lubricated and boxed up.","2021-06-22T23:59:35","","Completed","2021-06-04T23:59:35","No","No","No","Internal"]
[null,null,null,19998,null,"45_18/06/2021 14:07:48","2021-05-30T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ER vent fans Housing – rust weepings and filter frames rusted","Miscellaneous","General Appearance","External Factors","11.7","High","","","ER vent fans Housing  - Derusting/ buffing  followed by 2 coat primer & Full final coat painting completed.","2021-06-28T23:59:35","","Completed","2021-06-14T23:59:35","No","No","No","Internal"]
[null,null,null,20077,null,"45_15/07/2021 3:11:15 PM","2021-06-28T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Main engine unit 6 fuel pump barrel sealing ring leaking.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Main engine unit 6 fuel pump changed with spare fuel pump. ","2021-09-22T23:59:35","","Completed","2021-08-22T23:59:35","No","No","No","Internal","Noted awaiting next opportunity."]
[null,null,null,20076,null,"45_15/07/2021 3:24:45 PM","2021-06-29T23:59:35","Defect","Ship Staff","Ship Staff Insp.","COPT no 3 auto grease cup is having crack.","Cargo Mach.","Eng. / Strg. Comp.","Equipment Related","8.8","Medium","","","renewed with new spare","2021-10-07T23:59:35","SCAN210140","Completed","2021-09-30T23:59:35","No","No","No","Internal","Spares on order and will be arranged at next available opportunity. Target date revised accordingly."]
[null,null,null,20078,null,"45_15/07/2021 3:16:05 PM","2021-07-02T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Bilge pump priming unit, auto valve bellow leaking.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Bilge pump priming unit auto valve  renewed.","2021-10-23T23:59:35","SCAN210139","Completed","2021-10-24T23:59:35","No","No","No","Internal","Spares will be arranged once ready. Understand pump is operational now. Target date revised."]
[null,null,null,20079,null,"45_15/07/2021 3:39:24 PM","2021-07-02T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Hot water calorifier steam controller is malfunctioning.","Accommodation,Miscellaneous","MLC Related","Equipment Related","10.32","Very High","","","Renewed with new spare","2021-10-07T23:59:35","SCAN210141","Completed","2021-09-30T23:59:35","No","No","No","Internal","Spares on order and will be connected at next opportunity.\nTarget date revised accordingly."]
[null,null,null,20223,null,"45_31/07/2021 3:45:31 PM","2021-07-12T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Steering gear system forward port ram seal is leaking and all there steering pumps are dragging during emcy manual steering mode.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Technician came onboard, changed the seal for no:-2 ram port fwd and dragging issue sorted out.","2021-10-23T23:59:35","","Completed","2021-08-09T23:59:35","No","No","No","Internal"]
[null,null,null,20385,null,"45_15/08/2021 9:19:43 PM","2021-08-04T23:59:35","Observation","Ship Staff","Ship Staff Insp.","OXYGEN/ACETYLENE hose connection secured with jublie clips. it need to be secured with ear clamps.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","oxy/acetelyne hose secured with ear clamp","2021-11-17T23:59:35","SCAN210172","Completed","2021-08-12T23:59:35","No","No","No","Internal"]
[null,null,null,20386,null,"45_15/08/2021 9:12:43 PM","2021-08-05T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Main engine local manouvering engine telegraph system, new command couldn't able to accept and internal failure alarm persist. After tapping the control box, internal failure alarm disappear.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Local manouvering panel card renewed with new spare.","2021-11-17T23:59:35","","Completed","2021-08-18T23:59:35","No","No","No","Internal","Spares will be supplied in Singapore."]
[null,null,null,20820,null,"45_15/09/2021 9:33:18 PM","2021-08-06T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Air condition plant NO:-2 compressor MCCB short circuited.","E/R - Aux. Mach.,Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","renewed with new spare.","2021-12-22T23:59:35","SCAN210189","Completed","2021-10-02T23:59:35","No","No","No","Internal"]
[null,null,null,20664,null,"45_27/08/2021 16:20:13","2021-08-09T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Exhaust pipes on funnel to be derusted and painted at available opportunity","E/R - Pipes/ valves & fittings","General Appearance","External Factors","11.1","High","","","Scrapping, Cleaning followed by painting of Exhaust pipes on funnel carried out.","2021-11-08T23:59:35","","Completed","2021-08-30T23:59:35","No","No","No","Internal"]
[null,null,null,20665,null,"45_27/08/2021 16:04:46","2021-08-09T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Port & Stbd windlass anchor hydraulic brake is set wrongly.","Deck - Mooring Machinery","Mooring","Equipment Related","9.14","Medium","","","brake adjusted and matched wih the indicator and tried out, found satisfactory.","2021-11-08T23:59:35","","Completed","2021-09-16T23:59:35","No","No","No","Internal"]
[null,null,null,20666,null,"45_27/08/2021 16:12:37","2021-08-09T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Two of the gratings at port side manifold needs to renew. Other needs to derust and paint.","Deck - Pipe / Fittings","General Appearance","External Factors","11.1","High","","","2 gratings at port  side cargo manifold drip tray renewed, Derusting/ painting of Port manifold drip tray grating & drip tray completed. ","2021-08-29T23:59:35","","Completed","2021-08-26T23:59:35","No","No","No","Internal"]
[null,null,null,20667,null,"45_27/08/2021 16:14:40","2021-08-09T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Both pump room blower casing to derust and paint.","Deck - Pipe / Fittings","General Appearance","External Factors","11.1","High","","","Derusting / buffing followed by  Painting & highlighting of Port & Stbd pumproom blower casing completed.","2021-11-08T23:59:35","","Completed","2021-09-01T23:59:35","No","No","No","Internal"]
[null,null,null,20668,null,"45_31/08/2021 11:42:37 AM","2021-08-09T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Stbd line ME lube oil bunker pipe line has pin hole. ","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","Equipment Related","11.4","Very High","","","Defective section renewed with new pipe section.","2021-09-12T23:59:35","","Completed","2021-08-30T23:59:35","No","No","No","Internal"]
[null,null,null,20669,null,"45_31/08/2021 11:47:58 AM","2021-08-09T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Rusted and wasted material of Rain protector for port side funnel door at E/R blower platform ","Miscellaneous","Structural Condn. / WT integrity ","Equipment Related","11.8","Low","","","defective area renewed with new plates.","2021-09-12T23:59:35","","Completed","2021-08-30T23:59:35","No","No","No","Internal"]
[null,null,null,20670,null,"45_31/08/2021 11:59:42 AM","2021-08-09T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Water in oil sensor is suspected to be defective. to check and rectify.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","water in oil sensor replaced with new spare, present reading 0.14 locally ,now working in good order","2021-11-22T23:59:35","SCAN210178","Completed","2021-10-31T23:59:35","No","No","No","Internal","Spares already supplied. Install at next port. Target date revised."]
[null,null,null,17855,null,"45_16/02/2021 1:03:54 PM","2021-08-09T23:59:35","Defect","Ship Staff","Ship Staff Insp.","M/E viscosity steam auto control valve malfunctioning, valve need to overhaul.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","valve gear parts opened and inspected again all were in good order,cams for the limitswitches re adjusted,one of the limit switches was showing open circuit same repaired by re soldering,valve tried out by varing the viscocity from the controller in the ECR and operation was found to be satisfactory.","2021-11-22T23:59:35","","Completed","2021-11-01T23:59:35","No","No","No","Internal","What is RO no for this?"]
[null,null,null,20671,null,"45_31/08/2021 12:02:35 PM","2021-08-09T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Both air con controller is very old and worn condition.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","11.1","High","","","NO:-1 and 2 AC compressor panel  controller card renewed.","2021-11-22T23:59:35","SCAN215059","Completed","2021-11-02T23:59:35","No","No","No","Internal","On order. Will be supplied once ready. Target date revised."]
[null,null,null,20672,null,"45_31/08/2021 12:08:40 PM","2021-08-09T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","CCTV onboard is not yet commisioned.","Miscellaneous","Communication","Equipment Related","11.1","High","","","installation completed","2021-10-23T23:59:35","","Completed","2021-08-31T23:59:35","No","No","No","Internal"]
[null,null,null,20673,null,"45_31/08/2021 1:09:22 PM","2021-08-09T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","BWTS panel near calorifier is not secured properly. ","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","6.21","High","","","frames fabricated and welded to the BWTS panel.","2021-09-12T23:59:35","","Completed","2021-08-26T23:59:35","No","No","No","Internal"]
[null,null,null,20674,null,"45_27/08/2021 16:07:44","2021-08-09T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Oil level in windlass gear case is not visible. To top up.","Deck - Mooring Machinery","Mooring","External Factors","9.14","Medium","","","Gear oil Renewed for P & S windlass gear case.","2021-08-16T23:59:35","","Completed","2021-08-16T23:59:35","No","No","No","Internal"]
[null,null,null,20675,null,"45_27/08/2021 16:17:47","2021-08-09T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Rust weep marks below the cable tray on main deck. To be attended","Deck - Pipe / Fittings","General Appearance","External Factors","11.1","High","","","Derusting / buffing followed by painting carried out at the rust weep marks. ","2021-09-22T23:59:35","","Completed","2021-08-22T23:59:35","No","No","No","Internal"]
[null,null,null,20676,null,"45_31/08/2021 11:24:27 AM","2021-08-09T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","EGCS ventilation louver to be fitted with wheel and to ease up.","Miscellaneous","ISM Related","Equipment Related","10.32","Very High","","","Wheel fabricated and operating hanle interchanged with wheel. After changing the hand wheel, flaps ease up.","2021-08-23T23:59:35","","Completed","2021-08-19T23:59:35","No","No","No","Internal"]
[null,null,null,20677,null,"45_31/08/2021 11:53:42 AM","2021-08-09T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Some bunker pipelines at break of accomodation are marked with paint marker. same to be stenciled.","Deck - Pipe / Fittings","General Appearance","Human Error","11.4","Very High","","","stencil work  carried out for bunker pipeline at break of accomodation.","2021-08-19T23:59:35","","Completed","2021-08-16T23:59:35","No","No","No","Internal"]
[null,null,null,20678,null,"45_31/08/2021 12:18:31 PM","2021-08-09T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Steering gear pump need to paint.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.43","Medium","","","Steering gear pump painting work carried out.","2021-09-09T23:59:35","","Completed","2021-08-18T23:59:35","No","No","No","Internal"]
[null,null,null,20679,null,"45_31/08/2021 12:34:49 PM","2021-08-09T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Stbd DG FO filter lagging to renew.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.19","Very High","","","Stbd DG  FO filter lagging fixed properly and additional lagging used.","2021-08-16T23:59:35","","Completed","2021-08-14T23:59:35","No","No","No","Internal"]
[null,null,null,20680,null,"45_31/08/2021 12:40:47 PM","2021-08-09T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Atmospheric drain valve wheel and cap missing.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Spare wheel and cap fixed in valve.","2021-08-16T23:59:35","","Completed","2021-08-13T23:59:35","No","No","No","Internal"]
[null,null,null,20681,null,"45_31/08/2021 12:51:29 PM","2021-08-09T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ME liner tool is lying unsecured.","Miscellaneous","General Appearance","Human Error","10.29","Medium","","","ME liner tool secured.","2021-08-16T23:59:35","","Completed","2021-08-13T23:59:35","No","No","No","Internal"]
[null,null,null,20682,null,"45_31/08/2021 12:58:36 PM","2021-08-09T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Various weather tight doors of EGCS room and entrance to engine room does not have open close marking","Miscellaneous","General Appearance","Behaviour Based,Human Error","11.4","Very High","","","Open, shut marking painted in EGCS doors","2021-08-16T23:59:35","","Completed","2021-08-11T23:59:35","No","No","No","Internal"]
[null,null,null,20683,null,"45_31/08/2021 1:06:59 PM","2021-08-09T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Old and removed main air compressor body to shift to safe location.","E/R - Air Comp.","General Appearance","Equipment Related","10.29","Medium","","","Old and removed main air compressor body shifted to safe location top of ECR.","2021-08-22T23:59:35","","Completed","2021-08-14T23:59:35","No","No","No","Internal"]
[null,null,null,20684,null,"45_31/08/2021 1:11:47 PM","2021-08-09T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ME Air cooler U-tube manometer is empty.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Liquid filled up in U-tube manometer","2021-08-16T23:59:35","","Completed","2021-08-14T23:59:35","No","No","No","Internal"]
[null,null,null,20821,null,"45_15/09/2021 9:26:54 PM","2021-08-29T23:59:35","Defect","Ship Staff","Ship Staff Insp.","NO:-2 HFO purifier water block is faulty and purifier is not in use.","E/R - Purifier","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","water block replaced with new spare.","2021-12-18T23:59:35","","Completed","2021-12-05T23:59:35","No","No","No","Internal","Awaiting Readiness"]
[null,null,null,20822,null,"45_15/09/2021 9:44:18 PM","2021-09-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Vacuum toilet system vaccum control mechanism for few cabin toilets and engine room toilet found malfunctioning.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Required to renew the control mechanism, RO raised to keep some in spare.","2021-12-23T23:59:35","SCAN210188","Completed","2021-09-03T23:59:35","No","No","No","Internal"]
[null,null,null,20823,null,"45_15/09/2021 9:48:33 PM","2021-09-03T23:59:35","Observation","Ship Staff","Ship Staff Insp.","IG inlet valve to scrubber, 5/2 way direction control valve found leaking. ","E/R - Pipes/ valves & fittings,Inert Gas","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","5/2 way valve opened and inspected, telfon seals got damaged. required to renew the valve. RO raised.","2021-12-21T23:59:35","SCAN210173","Completed","2021-10-04T23:59:35","No","No","No","Internal"]
[null,null,null,20824,null,"45_15/09/2021 9:41:22 PM","2021-09-05T23:59:35","Defect","Ship Staff","Ship Staff Insp.","ME fuel oil auto back wash filter. diversion filter element found damaged during maintenance. spacer found crack near the stud securing slot.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Spacer renewed with new spare, for diversion filter element RO raised for same to keep in spare.","2021-12-20T23:59:35","SCAN210187","Completed","2021-09-06T23:59:35","No","No","No","Internal"]
[null,null,null,20825,null,"45_15/09/2021 9:37:27 PM","2021-09-07T23:59:35","Defect","Ship Staff","Ship Staff Insp.","In Engine control room NO:-2 440V feeder panel Air condition plant no:-2 compressor circuit breaker short circuited.","E/R - Aux. Mach.,Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","shunt coil taken from old breaker and fitted .Tested the Prefential trips  and found it in good working condition.","2021-12-23T23:59:35","SCAN210189","Completed","2021-11-12T23:59:35","No","No","No","Internal","Spare On order."]
[null,null,null,21290,null,"45_26/9/2021 8:52:18 PM","2021-09-18T23:59:35","Defect","Ship Staff","Ship Staff Insp.","NO # 2 Purifier friction pad parallel pin renewal for the motor drive unit.","E/R - Purifier","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","damaged friction pad parallel pin threads re dressed and tightened with thread lock.New Clutch drum received and renewed.Purifier tested,satisfactory.Put in operation","2022-02-20T23:59:35","SCAN210212","Completed","2022-02-28T23:59:35","No","No","No","Internal",""]
[null,null,null,20819,null,"45_15/09/2021 9:29:58 PM","2021-09-23T23:59:35","Defect","Ship Staff","Ship Staff Insp.","A/E 1,2,3 jacket water high temperature thermostat found malfunctioning. operation of thermostat is eratic.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Thermostat renewed, working satisfactory.","2022-01-23T23:59:35","","Completed","2022-01-21T23:59:35","No","No","No","Internal","readiness is end Nov."]
[null,null,null,21620,null,"45_13/10/2021 14:48:31","2021-09-27T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","No 7 foam monitor found leaking from flange.","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.35","Medium","","","No 7 foam monitor was removed from position,  cold work was done on the face of the leaking flange then smoothened . Same tested and no leaks observed .","2021-11-22T23:59:35","","Completed","2021-10-28T23:59:35","No","No","No","Internal","To be attended on priority basis"]
[null,null,null,21621,null,"45_14/10/2021 11:13:23 AM","2021-09-27T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","IGG panel to renew","E/R - Aux. Mach.,Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Panel renewed with new spare and IGG fired and tested all was found in good order O2 3.6 recorded .","2021-11-17T23:59:35","","Completed","2021-10-07T23:59:35","No","No","No","Internal"]
[null,null,null,21622,null,"45_14/10/2021 11:17:42 AM","2021-09-27T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","The air duct above ME to clean and paint.","Miscellaneous","Eng. / Strg. Comp.","External Factors","11.13","Low","","","Cleaning and painting carried out.","2022-01-22T23:59:35","","Completed","2021-12-30T23:59:35","No","No","No","Internal","Target date revised as work is in progress."]
[null,null,null,21623,null,"45_14/10/2021 11:22:11 AM","2021-09-27T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Sewage treatment plant blower casing is damaged, need to renew.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Repair work carried out.Now all in good order.","2022-01-11T23:59:35","SCAN210131","Completed","2021-12-14T23:59:35","No","No","No","Internal"]
[null,null,null,21624,null,"45_14/10/2021 11:44:00 AM","2021-09-27T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ODME spare as recommended by service engineer to renew.","Miscellaneous","MARPOL Related","Equipment Related","6.14","High","","","The zener barrier and the pressure switch has been replaced and ODME tried out in simulation mode and all found in good order.  ","2021-12-07T23:59:35","","Completed","2021-10-08T23:59:35","No","No","No","Internal"]
[null,null,null,21625,null,"45_14/10/2021 11:48:53 AM","2021-09-27T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","The vent head of hotwell in china passage to clean and painty","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.6","Medium","","","The vent head of hotwell cleaned and painted","2022-01-23T23:59:35","","Completed","2022-01-09T23:59:35","No","No","No","Internal","Now vessel is in port. Complete tit."]
[null,null,null,21626,null,"45_14/10/2021 11:51:30 AM","2021-09-27T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Elevator door closure motor is making noise and bearing need to renew.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Elevator cage door closing motor overhauled, bearings replaced with new spare.","2021-11-03T23:59:35","","Completed","2021-10-11T23:59:35","No","No","No","Internal"]
[null,null,null,21628,null,"45_13/10/2021 14:53:55","2021-09-27T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Lowering handle of Stbd lifeboat is thinned down at one location. To repair.","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.29","High","","","Lowering handle of Stbd lifeboat repaired.","2021-10-06T23:59:35","","Completed","2021-10-05T23:59:35","No","No","No","Internal"]
[null,null,null,21629,null,"45_13/10/2021 15:21:24","2021-09-27T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Crew smoke room carpet to clean","Accommodation","General Appearance","External Factors","11.13","Low","","","Cleaning of Crew smoke room carpet carried out.","2021-10-13T23:59:35","","Completed","2021-10-07T23:59:35","No","No","No","Internal"]
[null,null,null,21630,null,"45_13/10/2021 15:15:13","2021-09-27T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Antiskid mat to lay on both bridge wing.","Miscellaneous","General Appearance","Behaviour Based","5.47","Medium","","","Antiskid Rubber mats put in place at both bridge wings.","2021-10-11T23:59:35","","Completed","2021-10-05T23:59:35","No","No","No","Internal"]
[null,null,null,21627,null,"45_14/10/2021 12:01:47 PM","2021-10-02T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Fresh water tank level gauge is not working properly.","Elect. Mach. & Equip.,Hull & Tanks","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Sensor renewewd, level gauge working satisfactory","2022-02-20T23:59:35","SCAN210217","Completed","2022-02-06T23:59:35","No","No","No","Internal","Yet to get quotation"]
[null,null,null,22268,null,"45_19/10/2021 20:09:54","2021-10-11T23:59:35","Observation","Ship Staff","Ship Staff Insp.","6 Number of Loose stud found on stbd anchor chain; Namely between kenter joining shackle 5 & 4 – 4 studs; between kenter joining shackle 3 & 2 – 2 studs","Deck - Mooring Machinery","Mooring","Equipment Related","9.21","Medium","","","Loose stud to be welded in place after getting concurrence for hotwork from office. The job has been deferred to drydock and the same has been updated in REFMAN for \"DEFECTS TO OFFICE 2021\"","2022-01-10T23:59:35","","Completed","2021-11-22T23:59:35","Yes","No","No","Internal"]
[null,null,null,22269,null,"45_01/11/2021 10:52:33 AM","2021-10-23T23:59:35","Defect","Ship Staff","Ship Staff Insp.","ME  main control air line pipe leakage as crak was noticed at the pipe  weld seam area.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","External Factors","10.32","Very High","","","Leak rectified by doing hot work.","2021-11-17T23:59:35","SCAN210187","Completed","2021-10-27T23:59:35","No","No","No","Internal","Attend on priority basis."]
[null,null,null,22270,null,"45_01/11/2021 23:45:56","2021-10-23T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Sea water inlet pipe for deck seal, on deck found to be heavily corroded. Need to renew.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.27","Medium","","","The corroded section of pipe was replaced with the newly fabricated pipe","2021-12-22T23:59:35","","Completed","2021-11-11T23:59:35","No","No","No","Internal","Attend this on priority basis."]
[null,null,null,22567,null,"45_16/11/2021 3:31:13","2021-10-25T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Seawater supply to deck seal pipe on deck found to fully wasted, new pipe to be fabricated and replaced","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.27","Medium","","","The corroded section of pipe was replaced with the newly fabricated pipe","2021-12-23T23:59:35","","Completed","2021-11-11T23:59:35","No","No","No","Internal","Plan for same at the first opportunity."]
[null,null,null,22568,null,"45_16/11/2021 3:35:47","2021-10-25T23:59:35","Observation","Ship Staff","Ship Staff Insp.","IG to ballast line on deck found to have a soft patch, temporary repair found using plug and devcon","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.3","Very High","","","The complete length of pipe to be fabricated in drydock. The job has been added in REFMAN with all the details and photos","2022-01-24T23:59:35","","Completed","2022-01-09T23:59:35","Yes","No","No","Internal","To be planned at available opportunity.  Understand material is available."]
[null,null,null,23170,null,"45_20/12/2021 1:56:53 PM","2021-12-07T23:59:35","Non Conformity","Ship Staff","Ship Staff Insp.","THE IG MAIN LINE  LOW PRESSURE SWITCH FAULTY.","Inert Gas","Cargo / Ballast Systems","Equipment Related","10.32","Very High","","","PRESSURE SWITCH RENEWED WITH NEW SPARE RECEIVED","2022-01-22T23:59:35","","Completed","2022-01-06T23:59:35","No","No","No","Internal"]
[null,null,null,23294,null,"45_03/01/2022 21:33:07","2021-12-10T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Mooring winch hydraulic return line developed a hole, due to wastage of metal.","Deck - Mooring Machinery","Mooring","Equipment Related","9.14","Medium","","","The holed section of pipe was removed, new pipe fabricated and fitted back. Purging of the system carried out. Winch tested, no leaks observed.","2022-01-23T23:59:35","","Completed","2022-01-20T23:59:35","No","No","No","Internal"]
[null,null,null,23169,null,"45_20/12/2021 1:48:45 PM","2021-12-11T23:59:35","Defect","Ship Staff","Ship Staff Insp.","A/E Auto back wash filter change over valve not holding","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Complete change over unit renewed with new one.","2023-01-23T23:59:35","SCAN220165","Completed","2023-01-26T23:59:35","No","No","No","Internal"]
[null,null,null,23293,null,"45_3/01/2022 8:47:16 AM","2021-12-11T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","No #3 E/R fan Damper flap top half broke and fell on the fan impeller causing severe damage/pulverization of the impeller and resulted in breakage of the motor foundation.","Deck - Pipe / Fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Shore technician replaced the old damper and motor with new, counterweight and pneumatic levers welded onboard to shaft, now working satisfactory","2022-01-23T23:59:35","SCAN215083 .MOTOR REQ WILL BE MADE OFFICE SIDE","Completed","2022-01-03T23:59:35","No","No","No","Internal"]
[null,null,null,23295,null,"45_3/01/2022 9:04:55 AM","2021-12-12T23:59:35","Defect","Ship Staff","Ship Staff Insp.","INCINERATOR GARBAGE DOSING SIGHT GLASS BROKEN, AND THE SOLENOID VALVE FOR OPENING THE SLUICE DOOR LEAKING","Critical Equip.,Elect. Mach. & Equip.","MARPOL Related","Equipment Related","10.32","Very High","","","SOLENOID VALVE RECEIVED AND SAME RENEWED, TRIED OUT, WORKING SATISFACTORY","2022-01-22T23:59:35","SCAN210257","Completed","2022-01-03T23:59:35","No","No","No","Internal"]
[null,null,null,23296,null,"45_3/01/2022 8:53:24 AM","2021-12-20T23:59:35","Other","Ship Staff","Ship Staff Insp.","DG PRE HEATER CONTROLLER FAULTY","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","THE HEATER CONTROLLER REPLACED WITH NEW SPARE WORKING SATISFACTORY","2022-02-20T23:59:35","SCAN220007","Completed","2022-02-25T23:59:35","No","No","No","Internal"]
[null,null,null,23297,null,"45_3/01/2022 8:59:29 AM","2021-12-22T23:59:35","Defect","Ship Staff","Ship Staff Insp.","ME TOP BRACING NO #2 AIR LEAKGE FROM THE PRIMARY CHAMBER TO THE SECONDARY CHAMBERCAUSING THE POSITION PIN TO MOVE OUT.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","sPARES ON ORDER NEED TO BE OVERHAULED AND PRIMARY CHAMBER SEAL TO BE REPLACED .OTHER 3 TOP BRACINGS ARE IN GOOD ORDER.SPARES ON BOARD.TO BE TAKEN UP AT ANCHORAGE.CHECKED AND TOPPED UP WITH OIL.NEW PRESSURE GAUGE FITTED.THE INDICATOR IS IN NORMAL POSITIONWITH PRESSURE STEADY FOR MORE THAN 72 HOURS EXCEPT FOR MINOR SEEPAGE OF OIL.SO THIS DEFECT IS CLOSED.","2022-05-23T23:59:35","SCAN220002","Completed","2022-04-21T23:59:35","No","No","No","Internal"]
[null,null,null,23298,null,"45_3/01/2022 9:14:14 AM","2021-12-24T23:59:35","Defect","Ship Staff","Ship Staff Insp.","THE EGCS WASH WATER EFFLUENT ANALYZER SC1000 UNIT OUTPUT CARD IS DEFECTIVE.","Critical Equip.","MARPOL Related","Equipment Related","10.32","Very High","","","THE HMI PANEL IN ECR READINGS SHOWS OVER LIMIT.BUT THE LOCAL READINGS ARE CORRECT.REQUISITION RAISED FOR THE SAME.NEW PCB RECEIVED AND INSTALLED,SATISFACTORY","2022-03-20T23:59:35","SCAN220003","Completed","2022-04-01T23:59:35","No","No","No","Internal"]
[null,null,null,23299,null,"45_3/01/2022 9:17:59 AM","2021-12-26T23:59:35","Defect","Ship Staff","Ship Staff Insp.","AIR CON CONDENSER PIPING RUBBER VIBRATION DAMPER BELLOW  CONDITION HAS DETERIORATED, HAVE HEAT CRACKS.","E/R - Pipes/ valves & fittings,Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","HAVE TO BE REPLACED SPARE ON ORDER.RUBBER EXPANSION BELLOW RENEWED","2022-03-20T23:59:35","SCAN220008","Completed","2022-04-04T23:59:35","No","No","No","Internal"]
[null,null,null,23300,null,"45_3/01/2022 9:23:46 AM","2021-12-26T23:59:35","Defect","Ship Staff","Ship Staff Insp.","AUX BOILER NO #2 FEED WATER CONTROLLER FOR HIGH MODE OPERATION POSITIONER FAULTY LEVEL NOT MAINTAINING IN AUTO MODE","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","POSITIONER RECALIBRATED, NOW FOUND TO BE WORKING SATISFACTORY, NEW POSITIONER RECEIVED KEPT AS SPARE","2022-01-23T23:59:35","SCAN220004","Completed","2022-01-02T23:59:35","No","No","No","Internal"]
[null,null,null,23780,null,"45_01/02/2022 11:17:58 AM","2022-01-01T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Oil mist detector for engine room found to be in setting mode","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","defective detectors changed with new received","2022-05-23T23:59:35","SCAN220020","Completed","2022-05-12T23:59:35","No","No","No","Internal",""]
[null,null,null,23539,null,"45_15/01/2022 2:58:15 PM","2022-01-01T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Boiler main panel handle is missing","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Handles fixed back","2022-03-01T23:59:35","","Completed","2022-01-12T23:59:35","No","No","No","Internal"]
[null,null,null,23540,null,"45_15/01/2022 3:04:54 PM","2022-01-01T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Atmospheric condenser sea water inlet pipe one section is temporarily repaired","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","New section fabricated and fixed back","2022-02-07T23:59:35","","Completed","2022-01-12T23:59:35","No","No","No","Internal"]
[null,null,null,23541,null,"45_15/01/2022 3:11:08 PM","2022-01-01T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Sacrificial flange of port LT cooler leaking","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","sacrificial flange found damaged same removed and copper distance piece fitted, no leakages observed in operation.","2022-05-23T23:59:35","SCAN220016","Completed","2022-06-17T23:59:35","No","No","No","Internal","Flange will be supplied in Singapore."]
[null,null,null,23542,null,"45_15/01/2022 3:29:42 PM","2022-01-01T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Paint of bulkhead near stbd boiler burner top found in cracked condition due to high temp od sludge holding tank","Miscellaneous","Eng. / Strg. Comp.","External Factors","10.32","Very High","","","Old paint scrapped, cleaned and repainted","2022-01-23T23:59:35","","Completed","2022-01-14T23:59:35","No","No","No","Internal"]
[null,null,null,23543,null,"45_15/01/2022 3:50:48 PM","2022-01-01T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Incinerator milling pump found with leak marks","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Marks cleaned, painted and lagging renewed","2022-01-23T23:59:35","","Completed","2022-01-07T23:59:35","No","No","No","Internal"]
[null,null,null,23544,null,"45_15/01/2022 3:58:38 PM","2022-01-01T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Stbd boiler main steam stop valve leaking from gland","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Leak repaired by replacing with new gland","2022-02-01T23:59:35","","Completed","2022-01-14T23:59:35","No","No","No","Internal"]
[null,null,null,23545,null,"45_15/01/2022 4:00:52 PM","2022-01-01T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","OIl found collected in ME recess well","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.2","Low","","","Leak source to be identified, area to be cleaned.ME endcover bolts tightness checked and tightened.Area cleaned","2022-03-22T23:59:35","","Completed","2022-03-12T23:59:35","No","No","No","Internal"]
[null,null,null,23546,null,"45_15/01/2022 4:04:40 PM","2022-01-01T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Port LT cooler pressure gauge tapping plugged","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","instrument piece changed and new pressure gauge fitted.","2022-05-23T23:59:35","SCAN220019","Completed","2022-06-17T23:59:35","No","No","No","Internal"]
[null,null,null,23547,null,"45_15/01/2022 19:08:54","2022-01-01T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Various grating at manifold are holed and needs to be renewed.","Miscellaneous","General Appearance","Equipment Related","6.6","Medium","","","The gratings on both the manifolds were renewed with the newly received fiber gratings. Same secured with the locking arrangement.","2022-01-21T23:59:35","","Completed","2022-01-21T23:59:35","No","No","No","Internal"]
[null,null,null,23548,null,"45_15/01/2022 19:12:17","2022-01-01T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","The conduit pipe for cable of Stbd midship  mast light to be renewed as same is badly corroded.","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.4","Very High","","","Conduit pipe de-rusted & painted. ","2022-03-20T23:59:35","","Completed","2022-03-17T23:59:35","No","No","No","Internal"]
[null,null,null,23549,null,"45_15/01/2022 3:17:35 PM","2022-01-01T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","FWG ejector pump stop switch damaged","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Switch renewed","2022-01-07T23:59:35","","Completed","2022-01-04T23:59:35","No","No","No","Internal"]
[null,null,null,23550,null,"45_15/01/2022 3:22:06 PM","2022-01-01T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Aux engine oil max filters not in operation","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","OIl max filters put in  operation","2022-01-01T23:59:35","","Completed","2022-01-01T23:59:35","No","No","No","Internal"]
[null,null,null,23551,null,"45_15/01/2022 3:55:30 PM","2022-01-01T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Light casing on engine room blower platform found filled with water","Elect. Mach. & Equip.","Structural Condn. / WT integrity ","Equipment Related","10.32","Very High","","","Water drained and cleaned, o- ring renewed","2022-01-06T23:59:35","","Completed","2022-01-06T23:59:35","No","No","No","Internal"]
[null,null,null,23781,null,"45_01/02/2022 4:46:55 PM","2022-01-14T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Pump room blower vibrations found to be abnormal under operation","Deck - Machinery","Cargo / Ballast Systems","Equipment Related","10.32","Very High","","","Blower casing found to be worn out, temorarily repaired by putting punch marks inside the casing.PO raised.VIBRATION FOUND REDUCED OVER PERIOD OF TIME.","2022-03-22T23:59:35","SCAN220018","Completed","2022-04-02T23:59:35","No","No","No","Internal"]
[null,null,null,23782,null,"45_31/01/2022 11:42:28","2022-01-18T23:59:35","Defect","Ship Staff","Ship Staff Insp.","During the routine maintenance on the stbd side provision crane, the oil gauge glass was observed to be leaking oil. Same opened up for inspection and found the gauge glass was broken.","Deck - Machinery","General Appearance","Equipment Related","8.5","Very High","","","New one received at singapore & replaced","2022-04-17T23:59:35","SCAN220017","Completed","2022-03-31T23:59:35","No","No","No","Internal"]
[null,null,null,23862,null,"45_14/02/2022 8:16:51 AM","2022-01-28T23:59:35","Observation","Ship Staff","Ship Staff Insp.","ME unit#2 and #6, VIT for fuel pumps found to be stuck","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","No.2 Unit VIT linkage eased up,under observation.No.6 unit lubricated,working well.","2022-03-23T23:59:35","","Completed","2022-02-27T23:59:35","No","No","No","Internal"]
[null,null,null,23863,null,"45_15/02/2022 8:30:18 AM","2022-02-01T23:59:35","Observation","Ship Staff","Ship Staff Insp.","SOx value not increasing for the EGCS system","E/R - Main Engine,Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Service engineer attended the issue changed IR-source and chopper motor , issue resolved now operational.","2022-05-23T23:59:35","SCAN225033","Completed","2022-05-11T23:59:35","No","No","No","Internal"]
[null,null,null,23864,null,"45_14/02/2022 8:24:03 AM","2022-02-02T23:59:35","Observation","Ship Staff","Ship Staff Insp.","LT temp found to be increasing during loaded voyage at 71  rpm","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","100 per LT coooler to be cleaned chemically, filter for same was cleaned before departure last port.Both LT filter chemical cleaning carried out.ME tested at 70.5 rpm with sea water temp 27 deg,temeperature was holding well at 36 deg c.","2022-03-23T23:59:35","","Completed","2022-03-05T23:59:35","No","No","No","Internal"]
[null,null,null,23865,null,"45_14/02/2022 8:42:29 AM","2022-02-03T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Stbd(Low) sea chest filter basket internal rubber coating found to be bulging.","E/R - Air Comp.,E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Rubber coating to be renewed, deferred to dry dock","2025-02-03T23:59:35","","Completed","2022-02-03T23:59:35","Yes","No","No","Internal"]
[null,null,null,23866,null,"45_14/02/2022 2:55:43 PM","2022-02-04T23:59:35","Defect","Ship Staff","Ship Staff Insp.","CO2 room fixed fire fighting extinguishing cabinet for pump room and engine room found to be broken","Critical Equip.","Safety / LSA / FFA","Equipment Related","5.4","High","","","Fabrication for temperory cabinet in progress, PO raised for new cabinets.Steel Cabinet fabricated and installed for pump room.E/R & P/R Cabinet renewed with new spare.","2022-03-23T23:59:35","SCAN220040","Completed","2022-04-05T23:59:35","No","No","No","Internal"]
[null,null,null,23868,null,"45_14/02/2022 2:22:16 PM","2022-02-05T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Shaft earthing device jubliee clip holding silver band found to be broken","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Jubilee clip renewed","2022-02-25T23:59:35","","Completed","2022-02-17T23:59:35","No","No","No","Internal"]
[null,null,null,23867,null,"45_15/02/2022 7:42:02 PM","2022-02-07T23:59:35","Defect","Ship Staff","Ship Staff Insp.","ER VENT FAN#4 MOTOR FOUND GIVING LOW INSULATION ALARM AND TRIPPED","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","MOTOR ISOLATED, INSULATION FOUND TO BE 0, MOTOR DISMANTLED AND CHECKED, FOUND TO BE BURNT, PO RAISED.NEW MOTOR RECEIVED AND FITTED IN PLACE.FAN ASSEMBLED AND TESTED,SATISFACTORY","2022-03-22T23:59:35","SCAN220047","Completed","2022-02-27T23:59:35","No","No","No","Internal","Motor will be supplied in Singapore."]
[null,null,null,24146,null,"45_21/02/2022 9:54:50","2022-02-09T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Gear for the Slop P (IG35) IG branch valve actuator was found damaged, actuator inoperational. Need to repalce the actuator.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.2","Medium","","","Slop Port IG isolation valve replaced","2022-05-08T23:59:35","SCAN220053","Completed","2022-05-17T23:59:35","No","No","No","Internal","Will be arranged supply."]
[null,null,null,24147,null,"45_21/02/2022 10:04:10","2022-02-13T23:59:35","Observation","Ship Staff","Ship Staff Insp.","The messenger rope & pick up rope for the Aft ETA was observed to be frayed, needs replacement.","Deck - Machinery","Safety / LSA / FFA","Equipment Related","9.28","Medium","","","RO - SCAN220026 raised for new messenger rope & pick up rope. Received at Singapore and the rope was replaced","2022-05-12T23:59:35","SCAN220026 ","Completed","2022-02-26T23:59:35","No","No","No","Internal"]
[null,null,null,24148,null,"45_01/03/2022 10:40:28 AM","2022-02-14T23:59:35","Observation","Ship Staff","Ship Staff Insp.","NO.2 Accomodation air conditioning unit performance found to be reduced","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","TEV(aft) renewed.Leak near disch valve rectified.AC put in use at 75% load.Under observation.AC put in use at 100%.Cabin temperature maintaining at 20-21 deg when ambient is 34 deg with sea water at 29 degc.","2022-03-02T23:59:35","","Completed","2022-02-24T23:59:35","No","No","No","Internal"]
[null,null,null,24149,null,"45_01/03/2022 10:59:15 AM","2022-02-15T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","Engine room vent fan motor#3, fell down in engine air duct casing during operation, causing fan and motor damage","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","New Motor recieved and fitted inplace after detailed investigations and RCA , PRE AND POST CHECKS CARRIED OUT AS REQUIRED ","2022-03-23T23:59:35",", WORKING SATISFACTORY","Completed","2022-03-03T23:59:35","No","No","No","Internal","Motor and fan will be supplied in Singapore."]
[null,null,null,24150,null,"45_02/03/2022 7:08:27 PM","2022-02-22T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Pin hole was found to be developed in OWS 3rd stage filter chamber casing","E/R - Aux. Mach.,Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Casing to be renewed.New spare casing replaced the damaged one.System tested,satisfactory","2022-03-12T23:59:35","","Completed","2022-03-16T23:59:35","No","No","No","Internal"]
[null,null,null,24320,null,"45_07/03/2022 14:42:49","2022-02-23T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Chain on the safety walkway on deck requires de-rusting","Miscellaneous","General Appearance","Equipment Related","11.8","Low","","","Walkway chain de-rusted & painted","2022-03-26T23:59:35","","Completed","2022-03-17T23:59:35","No","No","No","Internal"]
[null,null,null,24321,null,"45_07/03/2022 14:10:42","2022-02-23T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Power box for speaker phone on monkey island broken & tied with cable tie","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.16","Low","","","Permanent fixing of the power box.Defective JB renewed","2022-03-26T23:59:35","","Completed","2022-04-06T23:59:35","No","No","No","Internal"]
[null,null,null,24322,null,"45_07/03/2022 14:44:01","2022-02-23T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Focsle store requires to be arranged neatly","Accommodation","General Appearance","Behaviour Based","5.11","Low","","","F'clse store secured. Cleaned. Save all painted","2022-03-26T23:59:35","","Completed","2022-03-22T23:59:35","No","No","No","Internal"]
[null,null,null,24323,null,"45_07/03/2022 14:45:17","2022-02-23T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Oxygen room door latch is hanging","Accommodation","General Appearance","Equipment Related","11.5","Medium","","","Oxygen room door latch to be repaired.Latch repair completed","2022-03-26T23:59:35","","Completed","2022-03-18T23:59:35","No","No","No","Internal"]
[null,null,null,24324,null,"45_07/03/2022 14:49:18","2022-02-23T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Lifeboat davit requires proper greasing","LSA / FFA","Safety / LSA / FFA","Behaviour Based","5.28","Very High","","","Greasing of LB davit carried out","2022-03-26T23:59:35","","Completed","2022-03-19T23:59:35","No","No","No","Internal"]
[null,null,null,24325,null,"45_07/03/2022 14:53:05","2022-02-23T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Stbd side pilot ladder shifting winch not working effectively","Deck - Machinery","General Appearance","Equipment Related","5.47","Medium","","","Overhauedl the shifting winch motor for stbd side pilot ladder","2022-04-25T23:59:35","","Completed","2022-03-24T23:59:35","No","No","No","Internal"]
[null,null,null,24326,null,"45_07/03/2022 14:34:08","2022-02-23T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Ballast discharge pipe in PR to be painted","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","","","","","Ballast discharging elbow in PR painted after carrying of repair on the soft patch","2022-02-23T23:59:35","","Completed","2022-03-29T23:59:35","No","No","No","Internal"]
[null,null,null,24327,null,"45_06/03/2022 9:08:34","2022-02-23T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Nav Locker auto switch for light tied with cable tie.","Accommodation","Safety / LSA / FFA","Inappropriate Procedure","","","","","Removed the cable tie from limit switch","2022-03-26T23:59:35","","Completed","2022-02-25T23:59:35","No","No","No","Internal"]
[null,null,null,24328,null,"45_07/03/2022 14:39:39","2022-02-23T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Fresh water valve on main deck near 1C COT was found leaking","Deck - Pipe / Fittings","General Appearance","Equipment Related","","","","","Valve tightned & leak arrested","2022-03-26T23:59:35","","Completed","2022-02-25T23:59:35","No","No","No","Internal"]
[null,null,null,24329,null,"45_07/03/2022 14:27:28","2022-02-23T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Pin hole leak in BWTS filter drain pipe in PR","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","","","","","Leaking pipe removed to ER workshop & the section renewed","2022-03-26T23:59:35","","Completed","2022-03-02T23:59:35","No","No","No","Internal"]
[null,null,null,24330,null,"45_07/03/2022 14:20:38","2022-02-23T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Emergency light for lifeboat/ life raft rusted & not rotating properly","Deck - Pipe / Fittings","General Appearance","Equipment Related","","","","","De-rusting & painting of the same completed. The turn table is fully greased & moving freely","2022-03-26T23:59:35","","Completed","2022-03-02T23:59:35","No","No","No","Internal"]
[null,null,null,24331,null,"45_07/03/2022 14:19:00","2022-02-23T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Lifeboat fwd & aft gripes bottle screw corroded","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","De-rusting completed and painted","2022-03-26T23:59:35","","Completed","2022-03-02T23:59:35","No","No","No","Internal"]
[null,null,null,24332,null,"45_07/03/2022 14:13:43","2022-02-23T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Drain chocked on the accommodation on portside A-deck","Accommodation","General Appearance","Equipment Related","","","","","Chocking removed from the pipe by hammering externally","2022-03-26T23:59:35","","Completed","2022-02-24T23:59:35","No","No","No","Internal"]
[null,null,null,24333,null,"45_06/03/2022 9:15:34","2022-02-23T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Nav Locker garbage stored next to electrical items.","Accommodation","General Appearance","Inappropriate Procedure","","","","","Nav locker cleaned and arrnaged","2022-03-26T23:59:35","","Completed","2022-02-25T23:59:35","No","No","No","Internal"]
[null,null,null,24334,null,"45_07/03/2022 14:32:10","2022-02-23T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ODME line in PR found with oil stain near flange on lower platform","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","","","","","The flanges from where minor leak was observed were fully tightened. Oil stain on the flanges were cleaned & painted","2022-03-26T23:59:35","","Completed","2022-02-26T23:59:35","No","No","No","Internal"]
[null,null,null,24335,null,"45_07/03/2022 14:22:17","2022-02-23T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Lifeboat selflowering wire pulley shows signs of corrosion","LSA / FFA","General Appearance","Equipment Related","","","","","De-rusting & painting of the same completed","2022-03-26T23:59:35","","Completed","2022-03-02T23:59:35","No","No","No","Internal"]
[null,null,null,24336,null,"45_07/03/2022 14:47:40","2022-02-23T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Life boat embarkation ladder bottom rope is frading","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","Close up inspection of the rope carried out. Found in satisfactory condition","2022-03-26T23:59:35","","Completed","2022-03-04T23:59:35","No","No","No","Internal"]
[null,null,null,24337,null,"45_07/03/2022 14:36:03","2022-02-23T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Various lights in PR requires to be renewed","Elect. Mach. & Equip.","Safety / LSA / FFA","Equipment Related","","","","","Faulty lights in PR renewed","2022-03-26T23:59:35","","Completed","2022-02-28T23:59:35","No","No","No","Internal"]
[null,null,null,24338,null,"45_07/03/2022 14:25:43","2022-02-23T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Deck stores to be arranged","Accommodation","General Appearance","Behaviour Based","","","","","Deck store arranged & inventory taken","2022-03-26T23:59:35","","Completed","2022-03-03T23:59:35","No","No","No","Internal"]
[null,null,null,24339,null,"45_07/03/2022 14:24:05","2022-02-23T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Stencil on foam hose box amiss","LSA / FFA","Safety / LSA / FFA","Industry Issue","","","","","Foam hose box stencilling carried out","2022-03-26T23:59:35","","Completed","2022-03-06T23:59:35","No","No","No","Internal"]
[null,null,null,24340,null,"45_07/03/2022 14:15:57","2022-02-23T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Hinges for lifejacket safety box on portside LB deck broken. ","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","new hinge fitted for lifejacket box on portside LB deck","2022-03-26T23:59:35","","Completed","2022-03-05T23:59:35","No","No","No","Internal"]
[null,null,null,24341,null,"45_07/03/2022 14:51:26","2022-02-23T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Port lifeboat - Screw fitted on the engine cover is not secured","LSA / FFA","Safety / LSA / FFA","Behaviour Based","","","","","Screw tightned","2022-03-25T23:59:35","","Completed","2022-03-02T23:59:35","No","No","No","Internal"]
[null,null,null,24343,null,"45_07/03/2022 14:12:17","2022-02-23T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Stay wire for main mast to be inspected for condition","Accommodation","General Appearance","Equipment Related","","","","","Main mast stay wire inspected for condition. Greasing carried out. Wire is in good condition","2022-03-26T23:59:35","","Completed","2022-02-28T23:59:35","No","No","No","Internal"]
[null,null,null,24317,null,"45_06/03/2022 9:05:49","2022-02-23T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Suez Cabin wash basin drain line to be repaired","Accommodation","General Appearance","Equipment Related","11.13","Low","","","Old one replaced with new one","2022-04-25T23:59:35","DSCAN220065","Completed","2022-04-18T23:59:35","No","No","No","Internal"]
[null,null,null,24318,null,"45_07/03/2022 14:37:39","2022-02-23T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Mooring winch lever locking puns not in satisafactory condition","Deck - Mooring Machinery","Mooring","Equipment Related","9.15","Medium","","","MW pins de-rusted & painted","2022-03-26T23:59:35","","Completed","2022-03-18T23:59:35","No","No","No","Internal"]
[null,null,null,24319,null,"45_07/03/2022 14:41:11","2022-02-23T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","VRCS junction box on deck near mid ship area requires to be de-rusted","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.8","Low","","","Repairing of the VRCS boxes in progress as the sides were wasted due to corrosion were completed.","2022-04-25T23:59:35","","Completed","2022-04-25T23:59:35","No","No","No","Internal"]
[null,null,null,24342,null,"45_06/03/2022 9:18:11","2022-02-26T23:59:35","Breakdown,Observation","Ship Staff","Ship Staff Insp.","Pump room skylight cover hinges found broken.","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","Equipment Related","","","","","Remove the skylight cover to ER for permanent repair of hinges","2022-03-22T23:59:35","","Completed","2022-03-06T23:59:35","No","No","No","Internal"]
[null,null,null,24949,null,"45_03/04/2022 7:23:36 AM","2022-03-18T23:59:35","Defect","Ship Staff","Ship Staff Insp.","MAC NO.2 COUPLING RUBBER DAMAGED","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","WHILECHECKING FOR LOW INSULATION ISSUE ON MAC NO.2,OBSERVED RUBBERINSERT IN THE COUPLING DAMAGED.NEW COUPLING RUBBER RECEIVED AND REPLACED THE DEFECTIVE ONE.TESTED,SATISFACTORY","2022-03-30T23:59:35","220087","Completed","2022-04-06T23:59:35","No","No","No","Internal"]
[null,null,null,24944,null,"45_01/04/2022 12:44:23 PM","2022-03-20T23:59:35","Defect","Ship Staff","Ship Staff Insp.","NO.3 boiler feed water p/p aft side seal is having minor leak.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Mechanical seal changed, no leakages now.","2022-04-22T23:59:35","","Completed","2022-04-25T23:59:35","No","No","No","Internal"]
[null,null,null,24950,null,"45_01/04/2022 12:08:23 PM","2022-03-22T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Egcs system ovbd fwd discharge line at bottom platform is having minor leak.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","office informed,leakage minimized and under observation, shore assistance arranged for anchorage at singapore.shore techncian attended vessel and replaced the defectiove section.EGCS tested while vsl was underway after singapore,satisfactory","2022-04-02T23:59:35","","Completed","2022-03-30T23:59:35","No","No","No","Internal"]
[null,null,null,24945,null,"45_12/04/2022 15:32:33","2022-04-04T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Mast riser hydraulic valve- leaking from actuator due to worn out seal ring of the piston","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.11","Medium","","","Renewed the worn out seal ring of the piston. Tried out & found in order","2022-07-04T23:59:35","SCAN220098","Completed","2022-07-23T23:59:35","No","No","No","Internal"]
[null,null,null,24946,null,"45_12/04/2022 15:37:15","2022-04-04T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Lifeboats fwd & aft securing gripe wires eyes are not mechanically spliced type as per maker manual.","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.29","High","","","Replaced with the new one received in Singapore 19 May 2022","2022-07-04T23:59:35","SCAN220095","Completed","2022-05-15T23:59:35","No","No","No","Internal"]
[null,null,null,24947,null,"45_12/04/2022 15:40:24","2022-04-04T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Stripping pump discharge pressure transmitter faulty & requires replacement","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.8","Medium","","","Replaced the faulty transmitter.\nTested & found it to be operational.","2022-07-04T23:59:35","SCAN220092","Completed","2022-07-15T23:59:35","No","No","No","Internal"]
[null,null,null,24948,null,"45_12/04/2022 16:01:46","2022-04-04T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Tank overfill alarm on bridge front- Strobe light body broken from the securing screws","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.14","Very High","","","Spare received & Renewed","2022-07-04T23:59:35","","Completed","2022-07-19T23:59:35","No","No","No","Internal"]
[null,null,null,25239,60570,"45_Mon Apr 25 2022 22:05:07 GMT+0800","2022-04-17T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Cargo eductor suction press & discharge gauge showing wrong reading in CCR.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.8","Medium","","","Vessel checked the copper tubes from the eductor to the the transmitter. Found tubes choked with sludge. Tubes cleared by blowing air. Eductor is found working satisfactory ","2022-12-22T23:59:35","SCAN220186","Completed","2022-12-07T23:59:35","No","No","No","Internal"]
[null,null,null,25240,50096,"45_Mon Apr 25 2022 22:09:38 GMT+0800","2022-04-17T23:59:35","Observation","Ship Staff","Ship Staff Insp.","4S WBT main valve indicator transmitter in solenoid box is faulty. ","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.8","Medium","","","Potentiometer of 4S WBT renewed and tested, found working satisfactory.","2023-06-26T23:59:35","SCAN230015","Completed","2023-06-15T23:59:35","No","No","No","Internal"]
[null,null,null,25241,53707,"45_Mon Apr 25 2022 22:24:26 GMT+0800","2022-04-17T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Magnetic compass of Port Side Lifeboat showing defectives readings.","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.29","High","","","New one received at Singapore & replaced ","2022-07-16T23:59:35","","Completed","2022-05-18T23:59:35","No","No","No","Internal"]
[null,null,null,25242,12124,"0_Mon Apr 25 2022 22:29:19 GMT+0800","2022-04-17T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Foam Monitor no. 1 and 6 Valve leaking, Requires renewal of Valve since complete seat ring has been damaged.","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.35","Medium","","","Renewed with the new valve received in Singapore 19 May 2022.","2022-07-16T23:59:35","","Completed","2022-05-15T23:59:35","No","No","No","Internal"]
[null,null,null,25528,15427,"45_Tue May 24 2022 20:15:57 GMT+0800","2022-05-08T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Stbd side pump room blower excessive vibration","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","5.18","High","","","Stbd side pump room blower coupling renewed with spare received onboard. Blower tried out and found satisfactory. No excessive vibration noticed.","2022-08-23T23:59:35","SCAN220018","Completed","2022-08-02T23:59:35","No","No","No","Internal"]
[null,null,null,25520,94838,"45_Tue May 24 2022 19:29:14 GMT+0800","2022-05-11T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Stbd side navigation side light conduit pipe wasted. ","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.4","Very High","","","Renewed the pipe","2022-06-11T23:59:35","","Completed","2022-06-19T23:59:35","No","No","No","Internal"]
[null,null,null,25521,32777,"45_Tue May 24 2022 19:40:36 GMT+0800","2022-05-11T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Stbd windlass gear oil sump slightly emulsified. ","Deck - Mooring Machinery","Mooring","Equipment Related","9.14","Medium","","","Renewed gear oil","2022-06-11T23:59:35","","Completed","2022-05-29T23:59:35","No","No","No","Internal"]
[null,null,null,25522,74598,"45_Tue May 24 2022 19:43:33 GMT+0800","2022-05-11T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Drain pipe on portside lifeboat deck from A-deck to upp deck is wasted","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.4","Very High","","","Cropped & renewed the wasted section of drain pipe with hot work after taking permission from office.","2022-07-11T23:59:35","","Completed","2022-06-15T23:59:35","No","No","No","Internal"]
[null,null,null,25523,34741,"45_Tue May 24 2022 19:46:26 GMT+0800","2022-05-11T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Pump room light glass broken at bottom platform","Miscellaneous","General Appearance","Equipment Related","11.11","Very High","","","Replaced the broken glass","2022-06-11T23:59:35","","Completed","2022-05-29T23:59:35","No","No","No","Internal"]
[null,null,null,25524,67135,"45_Tue May 24 2022 19:53:10 GMT+0800","2022-05-11T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Cover of solenoid box 3 on deck found with wasted edges","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.4","Very High","","","Cover removed and wasted sections renewed in workshop by cropping and welding new sections.","2022-07-11T23:59:35","","Completed","2022-09-08T23:59:35","No","No","No","Internal"]
[null,null,null,25525,87605,"45_Tue May 24 2022 19:55:10 GMT+0800","2022-05-11T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","MW 20 operating platform wasted.","Deck - Mooring Machinery","General Appearance","Equipment Related","11.5","Medium","","","Repaired the wasted section with hot work. Hot work concurrence from office taken for the work","2022-07-11T23:59:35","","Completed","2022-06-15T23:59:35","No","No","No","Internal"]
[null,null,null,25526,65596,"45_Tue May 24 2022 20:01:09 GMT+0800","2022-05-11T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Manifold hydraulic valve inlet & outlet Stop valve found to be in poor condition","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.41","Medium","","","Vessel renewed all stop valves for manifold actuators. All valves tried out and purged as required. Found no leaks. Defect closed out.","2022-11-22T23:59:35","RO- SCAN220132","Completed","2022-11-17T23:59:35","No","No","No","Internal"]
[null,null,null,25527,62007,"45_Tue May 24 2022 20:07:15 GMT+0800","2022-05-11T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Provision store entrance door from galley requires to be renewed as it is bend","Miscellaneous","General Appearance","Equipment Related","11.6","Medium","","","Vessel inspected the door. Found no bents on the door. Door closing effectively without any issues.","2022-11-25T23:59:35","SCAN220136","Completed","2022-11-25T23:59:35","No","No","No","Internal"]
[null,null,null,25529,81025,"45_Thu May 26 2022 13:26:32 GMT+0800","2022-05-11T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Port side provision crane hydraulic hose ruptured","Deck - Machinery","Eng. / Strg. Comp.","Equipment Related","10.28","Low","","","Hose received and renewed with new hose.","2022-08-11T23:59:35","SCAN220183","Completed","2022-09-07T23:59:35","No","No","No","Internal"]
[null,null,null,25530,75604,"45_Thu May 26 2022 13:42:34 GMT+0800","2022-05-11T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Soot collecting is having temporary repairs at two places, need to change plate section.","Hull & Tanks","Eng. / Strg. Comp.","Equipment Related","10.31","Very High","","","hot work carried out ,steel plate section renewed with new plate. ","2022-06-22T23:59:35","","Completed","2022-06-16T23:59:35","No","No","No","Internal"]
[null,null,null,25531,79343,"45_Thu May 26 2022 13:47:04 GMT+0800","2022-05-11T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Sewage treatment plant no.1 blower body is completely wasted need replacement.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Blower renewed with new one.","2023-04-09T23:59:35","SCAN220133","Completed","2023-03-25T23:59:35","No","No","No","Internal"]
[null,null,null,25535,12779,"45_Thu May 26 2022 13:35:48 GMT+0800","2022-05-11T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","No.1 fwg evaporator side end plate cover is wasted need to replace.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","End plate cover and end  plates renewed.Found no leak.","2022-10-22T23:59:35","SCAN220129","Completed","2022-10-27T23:59:35","No","No","No","Internal"]
[null,null,null,25536,50475,"45_Tue May 24 2022 19:49:27 GMT+0800","2022-05-11T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Valve remote control system hydraulic pipe line leaking at 4C fwd area","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","11.4","Very High","","","Renewed the section of pipe by removing it to ER workshop.\nPressure testing carried out after renewal.","2022-05-22T23:59:35","","Completed","2022-05-16T23:59:35","No","No","No","Internal"]
[null,null,null,25538,82823,"45_Thu May 26 2022 13:22:41 GMT+0800","2022-05-11T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Retrofit air conditioning units are not put in use for various electrical panels.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Inappropriate Procedure","","","","","all retrofit units put in use after changing set points.","2022-05-23T23:59:35","","Completed","2022-05-16T23:59:35","No","No","No","Internal"]
[null,null,null,25539,22462,"45_Thu May 26 2022 13:31:34 GMT+0800","2022-05-11T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","steering gear room bilge drain valve is not operational. need to overhaul/replace.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","valve removed from place and overhauled and put in place, working satisfactory.","2022-06-22T23:59:35","","Completed","2022-05-18T23:59:35","No","No","No","Internal"]
[null,null,null,25540,32023,"45_Tue May 24 2022 19:27:31 GMT+0800","2022-05-11T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Portside navigation side light conduit pipe wasted & requires renewal","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.4","Very High","","","Renewed the pipe","2022-06-11T23:59:35","","Completed","2022-05-19T23:59:35","No","No","No","Internal"]
[null,null,null,25541,68807,"45_Tue May 24 2022 19:32:24 GMT+0800","2022-05-11T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Portside diesel oil manifold sample line wasted","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.4","Very High","","","Section removed and wasted section replaced with new one. Pressure tested to 6 bars.","2022-06-11T23:59:35","","Completed","2022-05-23T23:59:35","No","No","No","Internal"]
[null,null,null,25537,53789,"45_Tue May 24 2022 20:03:34 GMT+0800","2022-05-15T23:59:35","Observation","Ship Staff","Ship Staff Insp.","2P IG pressure sensor showing difference in value from normal by 4 mBar","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.13","Medium","","","Carried out Zero calibration of the pressure sensor & check for proper working.","2022-06-22T23:59:35","","Completed","2022-05-18T23:59:35","No","No","No","Internal"]
[null,null,null,25532,46961,"45_Thu May 26 2022 13:53:46 GMT+0800","2022-05-16T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","No.2 main air compressor lp stage piston and connecting rod found broken,need to be replaced.","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","all damaged parts replaced and compressor put back in use, working satisfactory.","2022-06-07T23:59:35","SCAN220134","Completed","2022-05-26T23:59:35","No","No","No","Internal"]
[null,null,null,25533,55411,"45_Thu May 26 2022 17:33:24 GMT+0800","2022-05-18T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Ship Staff Insp.","Emergency fire pump discharge line duo check valve (NRV) is Not water tight, need to overhaul/replacement.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Non return valve replaced with new spare received.\nPump Tried out working satisfactory.","2022-07-23T23:59:35","SCAN220137","Completed","2022-08-07T23:59:35","No","No","No","Internal"]
[null,null,null,25534,62901,"45_Sat May 28 2022 16:16:01 GMT+0800","2022-05-20T23:59:35","Observation","Ship Staff","Ship Staff Insp.","ODME overboard valve on deck near PR entrance- Stop valve for the actuator is in poor condition due to corrosion","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.11","Medium","","","Renewed the valve & tested. Found in order","2022-08-19T23:59:35","SCAN220132","Completed","2022-07-23T23:59:35","No","No","No","Internal"]
[null,null,null,25763,53755,"45_Tue Jun 14 2022 16:03:59 GMT+0800","2022-05-24T23:59:35","Defect","Ship Staff","Ship Staff Insp.","EGCS sea water pump discharge line is having pin hole after the discharge valve.","E/R - Aux. Mach.,E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Permanent repair carried out by welding  ","2022-07-23T23:59:35","","Completed","2022-07-25T23:59:35","No","No","No","Internal"]
[null,null,null,26020,63240,"45_Mon Jun 20 2022 13:59:33 GMT+0800","2022-06-12T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Port & stbd side manifold drip tray drain line to 4P & 4S COT were observed to be corroded & wasted","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","11.4","Very High","","","Removed to work shop & renewed.","2022-06-22T23:59:35","","Completed","2022-06-20T23:59:35","No","No","No","Internal"]
[null,null,null,26019,27385,"45_Thu Jun 30 2022 15:40:08 GMT+0800","2022-06-17T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Port side lt cooler no sacrificial flange installed in inlet sea water  pipe line.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","External Factors,Equipment Related","10.31","Very High","","","new instrument piece fitted with sacrificial flange..","2022-07-23T23:59:35","SCAN220019","Completed","2022-07-19T23:59:35","No","No","No","Internal"]
[null,null,null,26018,19275,"45_Thu Jun 30 2022 15:34:30 GMT+0800","2022-06-21T23:59:35","Defect","Ship Staff","Ship Staff Insp.","sewage holding tank sea water flushing line for level floats found leaking.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.31","Very High","","","pipe section renewed with new fabricated pipe.","2022-07-02T23:59:35","","Completed","2022-06-24T23:59:35","No","No","No","Internal"]
[null,null,null,26316,64345,"45_Fri Jul 22 2022 19:13:26 GMT+0800","2022-06-28T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","EGCS inlet water analyzer turbidity sensor damaged due to water ingress.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Sensor received and renewed, Sensor configured and tried out - working  satisfactory. ","2022-09-07T23:59:35","SCAN220167","Completed","2022-08-10T23:59:35","No","No","No","Internal"]
[null,null,null,26317,74049,"45_Sat Jul 23 2022 13:15:54 GMT+0800","2022-06-29T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Aux engine fuel oil line pressure regulating valve near no.1 aux engine is having slight leakage.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Pressure regulating valve renewed with new one.","2023-01-23T23:59:35","SCAN220124","Completed","2023-01-26T23:59:35","No","No","No","Internal"]
[null,null,null,26362,70483,"45_Wed Jul 27 2022 15:59:25 GMT+0800","2022-07-13T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","SEA WATER INLET VALVE TO IGG IS NOT WATER TIGHT NEED TO OVERHAUL/REPLACE","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","VALVE RENEWED.","2022-10-07T23:59:35","","Completed","2022-08-14T23:59:35","No","No","No","Internal"]
[null,null,null,26358,38857,"45_Mon Jul 25 2022 15:12:05 GMT+0800","2022-07-16T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Glass mirrors for cabin toilet need to be replaced","Accommodation","General Appearance","Equipment Related","","","","","Replace the mirrors in all cabin toilets on receipt of spare","2022-09-16T23:59:35","DSCAN220189","Completed","2022-08-21T23:59:35","No","No","No","Internal"]
[null,null,null,26359,38059,"45_Mon Jul 25 2022 15:16:03 GMT+0800","2022-07-16T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Battery room switch is broken on E-deck","Accommodation,Elect. Mach. & Equip.","General Appearance","Equipment Related","11.16","Low","","","Renewal in progress without hotwork. Switch body disconnected, base plate removed and being renewed. To be attached by nut & bolt onto the existing angle bar.","2022-08-16T23:59:35","","Completed","2022-08-03T23:59:35","No","No","No","Internal"]
[null,null,null,26361,75763,"45_Tue Jul 26 2022 12:27:06 GMT+0800","2022-07-17T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Rollers for Pilot ladder reel worn out","Deck - Machinery","ISM Related","Equipment Related","5.47","Medium","","","Vessel renewed Port & Stbd side pilot ladder wheels and carried out repairs on trackway. Stbd side pilot ladder reel completely de rusted and made operational. Same to be carried out on port side.","2022-12-17T23:59:35","SCAN220192","Completed","2022-11-25T23:59:35","No","No","No","Internal"]
[null,null,null,26491,63154,"45_Mon Aug 15 2022 19:42:53 GMT+0800","2022-07-18T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Oil detection alarm of ME jacket water not operational.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Sensor working alarm getting activated in A.M.S. Sensor put into use.","2022-08-18T23:59:35","","Completed","2022-08-09T23:59:35","No","No","No","Internal"]
[null,null,null,26492,63685,"45_Mon Aug 15 2022 19:50:56 GMT+0800","2022-07-18T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","The exhaust pipe passing from ER to EGCS room to seal.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Gap filled with lagging material and then using metal sheet on top of lagging material to secure it in place","2022-07-29T23:59:35","","Completed","2022-08-15T23:59:35","No","No","No","Internal"]
[null,null,null,26493,78805,"45_Mon Aug 15 2022 19:53:09 GMT+0800","2022-07-18T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Port side store to arrange properly and need to fabricate extra racks.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","NEW RACKS FABRICATED AND PUT INTO USE.","2022-09-18T23:59:35","","Completed","2022-08-15T23:59:35","No","No","No","Internal"]
[null,null,null,26494,18808,"45_Mon Aug 15 2022 19:55:04 GMT+0800","2022-07-18T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","COPT platform port side area tracing steam leakage to rectify.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Leak rectified.  ","2022-08-03T23:59:35","","Completed","2022-08-22T23:59:35","No","No","No","Internal"]
[null,null,null,26500,49802,"45_Mon Aug 15 2022 19:46:08 GMT+0800","2022-07-18T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Both IG blower drain lines to repair and area to clean.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Corroded pipe section and flexible hoses renewed.","2022-08-04T23:59:35","","Completed","2022-08-04T23:59:35","No","No","No","Internal"]
[null,null,null,26501,22202,"45_Mon Aug 15 2022 19:48:16 GMT+0800","2022-07-18T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ME Fuel pump umbrella spare glass to clean for all units.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Two units glasses renewed and remaining units glasses cleaned.","2022-08-08T23:59:35","","Completed","2022-07-24T23:59:35","No","No","No","Internal"]
[null,null,null,26360,87830,"45_Tue Jul 26 2022 11:50:34 GMT+0800","2022-07-18T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Garbage compactor hydraulic hoses sheathing damaged. ","Elect. Mach. & Equip.","General Appearance","Equipment Related","11.10","Medium","","","Hose has been replaced with a similar hose from the provision crane. The original hose when received shall be fixed back.","2022-09-17T23:59:35","SCAN220191","Completed","2022-07-29T23:59:35","No","No","No","Internal"]
[null,null,null,26753,26013,"45_Thu Sep 01 2022 17:58:24 GMT+0800","2022-07-20T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Ship Staff Insp.","Section of area in 5P WBT on 2nd stringer  found to have coating failure.","Hull & Tanks","Cargo / Ballast Systems","Equipment Related","2.9","Medium","","","Area to be chipped and painted with epoxy primer.","2022-08-24T23:59:35","","Completed","2022-08-24T23:59:35","No","No","No","Internal"]
[null,null,null,26363,29242,"45_Sun Jul 31 2022 18:53:29 GMT+0800","2022-07-22T23:59:35","Observation","Ship Staff","Ship Staff Insp.","VRCS hydraulic main line holed near 3C COT ","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","11.4","Very High","","","Remove & renew the section of leaking pipe ","2022-07-29T23:59:35","","Completed","2022-07-29T23:59:35","No","No","No","Internal"]
[null,null,null,26497,33459,"45_Sun Aug 07 2022 07:22:53 GMT+0800","2022-07-28T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Oil leaks observed from controller for winch M7","Deck - Machinery","Mooring","Equipment Related","9.14","Medium","","","Controller shaft \"O\" rings and step seals renewed. Leak arrested.","2022-07-28T23:59:35","","Completed","2022-07-28T23:59:35","No","No","No","Internal"]
[null,null,null,26495,28178,"45_Sun Aug 07 2022 07:18:46 GMT+0800","2022-07-29T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Oil leaks observed from controller for winch M16","Deck - Machinery","Mooring","Equipment Related","9.14","Medium","","","Renewed the o rings and step seals for the controller. Leak rectified.","2022-07-29T23:59:35","","Completed","2022-07-29T23:59:35","No","No","No","Internal"]
[null,null,null,26496,49505,"45_Sun Aug 07 2022 07:21:20 GMT+0800","2022-07-29T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Oil leaks observed form controller for winch M14","Deck - Machinery","Mooring","Equipment Related","9.14","Medium","","","Shaft \"O\" rings & step seals renewed and leak arrested.","2022-07-29T23:59:35","","Completed","2022-07-29T23:59:35","No","No","No","Internal"]
[null,null,null,26498,57009,"45_Sun Aug 07 2022 07:24:36 GMT+0800","2022-07-29T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Oil leaks observed from port windlass controller","Deck - Machinery","Mooring","Equipment Related","9.14","Medium","","","Vessel checked the controller and found in bad shape with heavy pitting. Renewed the controller with spare, renewed the shaft \"O\" rings and step seals.","2022-08-01T23:59:35","","Completed","2022-08-01T23:59:35","No","No","No","Internal"]
[null,null,null,26502,74090,"45_Sun Aug 07 2022 07:28:33 GMT+0800","2022-07-29T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Various sections of VRCS pipe line forward of midship area in bad shape on main deck with heavy rust & thinning down of pipe line thickness. ","Deck - Pipe / Fittings","Cargo / Ballast Systems","External Factors","11.4","Very High","","","Sections forward of midship area renewed/ repaired. Sections have been fixed back with new \"O\" rings and tried out. No leaks observed.","2022-08-04T23:59:35","","Completed","2022-08-05T23:59:35","No","No","No","Internal"]
[null,null,null,26499,36202,"45_Wed Aug 10 2022 06:39:55 GMT+0800","2022-07-31T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Devcon applied to high pressure flange on VRCS line to arrest the leak from the flange.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Inappropriate Procedure","11.4","Very High","","","Devcon removed and the \"O\" ring inside the flange renewed. Flange fixed back at position.","2022-08-01T23:59:35","","Completed","2022-08-01T23:59:35","No","No","No","Internal"]
[null,null,null,26752,51236,"45_Thu Sep 01 2022 17:28:47 GMT+0800","2022-08-10T23:59:35","Defect","Ship Staff","Ship Staff Insp.","During de-ballasting at load port, observed inlet pipe to WBP#2 holed.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.44","High","","","Pipe section removed from location. During build up in engine room found 11 locations where pitting was observed. Build up carried out and pipe fixed back at location and tested.","2022-08-27T23:59:35","","Completed","2022-08-25T23:59:35","No","No","No","Internal"]
[null,null,null,26832,59397,"45_Thu Sep 15 2022 16:25:00 GMT+0800","2022-09-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Tracing steam line inlet valves two nos  for auxiliary engine fuel oil lines found leaking from bonnet ","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Two valves bonnet packing renewed","2022-09-04T23:59:35","","Completed","2022-09-02T23:59:35","No","No","No","Internal"]
[null,null,null,26833,69116,"45_Thu Sep 15 2022 16:34:17 GMT+0800","2022-09-01T23:59:35","Observation","Ship Staff","Ship Staff Insp.","one number signal light column near boiler water circulating pump found not operational ","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Fault in the panel rectified","2022-09-12T23:59:35","","Completed","2022-09-04T23:59:35","No","No","No","Internal"]
[null,null,null,26829,28785,"45_Fri Sep 16 2022 13:54:51 GMT+0800","2022-09-08T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Cover for hydraulic Box #1 found wasted at sections","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.4","Very High","","","Cover removed (03 pcs). The edges were renewed with flat bars. Box covers chipped and painted and fixed back at location.","2022-09-22T23:59:35","","Completed","2022-09-18T23:59:35","No","No","No","Internal"]
[null,null,null,26830,78042,"45_Fri Sep 16 2022 13:57:45 GMT+0800","2022-09-08T23:59:35","Observation","Ship Staff","Ship Staff Insp.","VRCS pipe section (Return line) found thinned down at section near clamp. ","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","11.4","Very High","","","Vessel carried out repairs & renewals on thinned down and leaking return lines. 1 Full length delivery line renewed. VRCS line chipped and painted until midship area from forward.","2022-09-22T23:59:35","","Completed","2022-09-15T23:59:35","No","No","No","Internal"]
[null,null,null,27368,80618,"45_Tue Nov 01 2022 14:07:07 GMT+0800","2022-09-16T23:59:35","Observation","Ship Staff","Ship Staff Insp.","L.T.cooler no#2 inlet pipe chemical cleaning line was found leaking slightly.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Pipe removed from place,taken to workshop ,leaking pipe renewed.","2022-11-02T23:59:35","","Completed","2022-10-18T23:59:35","No","No","No","Internal"]
[null,null,null,27367,95517,"45_Wed Oct 19 2022 12:17:59 GMT+0800","2022-09-28T23:59:35","Defect","Ship Staff","Ship Staff Insp.","The sea water bypass valve for atmospheric condenser found not opening fully.Due to this the L.T. temperature for engine room was found to be going up to 39 deg when main engine RPM IS about 56 at sea water temperature of 32 deg.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.31","Very High","","","The valve was tried to be eased up by opening and shutting the valve. became normal after eased up,  now operating in a easy way.","2022-11-13T23:59:35","","Completed","2022-10-24T23:59:35","No","No","No","Internal"]
[null,null,null,27194,39058,"45_Wed Oct 12 2022 13:45:03 GMT+0800","2022-10-02T23:59:35","Non Conformity","Ship Staff","Ship Staff Insp.","Bridge wings not fitted with BNWAS repeaters alarm","Navigation - VDR / BNWAS","Navigation","Equipment Related","","","","","This regulation is applicable for ships where BANWAS was installed after 1st July 2011. This BANWAS is older than this and hence not applicable","2023-12-13T23:59:35","","Completed","2022-11-28T23:59:35","No","No","No","Internal"]
[null,null,null,27195,95018,"0_Wed Oct 12 2022 13:46:45 GMT+0800","2022-10-02T23:59:35","Defect","Ship Staff","Ship Staff Insp.","1 no window wiper not effective","Navigation - Others","Navigation","Equipment Related","","","","","Wiper disconnected, found belt worn out. Belt renewed and rollers renewed. Wiper fixed back and tried out. Found working.","2023-01-02T23:59:35","","Completed","2022-11-18T23:59:35","No","No","No","Internal"]
[null,null,null,27197,25916,"45_Wed Oct 12 2022 13:48:58 GMT+0800","2022-10-02T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","ECHO SOUNDER PRINTER ROTOR/ MOTOR ISSUE","Navigation - Echo Sounder / Speed Log","Navigation","Equipment Related","","","","","Echo sounder renewed with new during class annuals.","2023-01-02T23:59:35","","Completed","2022-10-22T23:59:35","No","No","No","Internal"]
[null,null,null,27196,93337,"45_Wed Oct 12 2022 13:43:03 GMT+0800","2022-10-04T23:59:35","Non Conformity","Ship Staff","Ship Staff Insp.","AFT WHISTLE tested with passing vessels: Decibels lower than recommended, Current Audible Range less than 1.2 NM","Navigation - Others","Navigation","Equipment Related","","","","","Vsl was able to confirm the range of aft whistle at 1.5 Nm with passing vessels . As per Annex III - technical specs of whistles , the range should be 2 Nm if only one whistle . Since vessel has combination of 2 whistles - F/A , the range of one whistle can be lesser than the other . The AFT whistle was overhauled and tested satisfactory. This job is therefore closed . ","2023-01-04T23:59:35","","Completed","2023-01-09T23:59:35","No","No","No","Internal"]
[null,null,null,27366,14591,"45_Wed Oct 19 2022 12:01:17 GMT+0800","2022-10-06T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","Ballast pump seal was found leaking  during ballasting operation,","Miscellaneous","Cargo / Ballast Systems","Equipment Related","8.44","High","","","Pump volute cover opened,found bearing locking ring pin broken, nut loose and bearing loose on shaft.Found shaft worn out by 0.2mm. Misalignment between intermediate shaft and pump was found to be 0.4 mm (horizontal). Shaft bearing resting area was punched marked and bearing fitted on shaft.Bearing was found to be  tight on shaft.Pump tried out  is running o.k. No leakage from seal. Requisition made for new shaft. Mech seal has been replaced with new spare, same  pump has been tried out, since now running in normal condition.","2022-11-06T23:59:35","REQ.NO:220249 DATED :18TH OCT 22","Completed","2022-10-09T23:59:35","No","No","No","Internal"]
[null,null,null,27662,79832,"45_Fri Nov 11 2022 09:38:50 GMT+0800","2022-10-07T23:59:35","Defect,Observation","Ship Staff","Ship Staff Insp.","BWTS NU pump #2 giving differential pressure alarm on operation and activating ESD on BWTS system","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","6.21","High","","","Vessel carried out cleaning of the NU pump dosing line. Overhauling of the back pressure valve & adjusting of NU pump strokes to 50 from the original 100. tried out at sea for 30 min and found satisfactory. Tried out again at load port and no differential pressure alarms were triggered.","2022-11-22T23:59:35","","Completed","2022-11-07T23:59:35","No","No","No","Internal"]
[null,null,null,27648,36714,"45_Thu Nov 10 2022 16:20:48 GMT+0800","2022-10-21T23:59:35","Breakdown","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Bosun store water mist system main panel showing fault alarm.To order required spares","LSA / FFA","Safety / LSA / FFA","Equipment Related","8.69","Medium","","","Spares renewed. Fault rectified.","2022-11-11T23:59:35","","Completed","2022-12-25T23:59:35","No","No","No","Internal"]
[null,null,null,27650,54764,"45_Wed Nov 09 2022 20:49:03 GMT+0800","2022-10-21T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Spare main engine fuel pump VIT  rack is stuck,spare pump needs to be o'hauled.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Spare fuel pump plunger and barrel assembly removed from pump. Sealing rings cleaned and fresh molykote spray applied.Oil applied on vit and fuel pump racks,boxed back and tried out.","2022-11-12T23:59:35","","Completed","2022-11-06T23:59:35","No","No","No","Internal"]
[null,null,null,27652,99686,"0_Wed Nov 09 2022 21:06:24 GMT+0800","2022-10-21T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Galley communitor not operational and the power panel of same not operational.","Accommodation","MARPOL Related","Equipment Related","11.13","Low","","","Power panel made operational by front cover for starter panel repairing. Disperator o'hauled completely with existing spare parts and made operational.","2022-11-22T23:59:35","","Completed","2022-11-14T23:59:35","No","No","No","Internal"]
[null,null,null,27654,63100,"45_Thu Nov 10 2022 16:15:40 GMT+0800","2022-10-21T23:59:35","Breakdown","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Oil spray was noted below port provision crane.To rectify leak ","Deck - Machinery","MARPOL Related","Equipment Related","8.50","Medium","","","One number hose was found leaking,same renewed,one more hose which was found damaged was also renewed","2022-11-04T23:59:35","","Completed","2022-10-30T23:59:35","No","No","No","Internal"]
[null,null,null,27658,70681,"0_Wed Nov 09 2022 21:14:57 GMT+0800","2022-10-21T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Two of the QMI OMD showing fault in the main panel,fault to rectify.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","5.35","Medium","","","Faulty detector replaced with new detector received.","2022-11-09T23:59:35","","Completed","2022-10-28T23:59:35","No","No","No","Internal"]
[null,null,null,27663,93369,"0_Wed Nov 09 2022 20:59:47 GMT+0800","2022-10-21T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","DG fuel oil supply pump no:1 leaking from seals,seal to be renewed ","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Pump checked,found leakage from pressure gauge tappings, leakage rectified.","2022-11-07T23:59:35","","Completed","2022-11-02T23:59:35","No","No","No","Internal"]
[null,null,null,27647,80287,"45_Wed Nov 09 2022 20:56:48 GMT+0800","2022-10-21T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","100% LT cooler sea water valves are not holding ,valve to be ordered and renewed.","Deck - Pipe / Fittings,E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.31","Very High","","","Spares received. Both Inlet and Outlet valves have been renewed and tested holding. ","2023-04-24T23:59:35","SCAN220260","Completed","2023-05-06T23:59:35","No","No","No","Internal"]
[null,null,null,27649,52858,"45_Fri Nov 11 2022 09:31:22 GMT+0800","2022-10-22T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Meat room door packing is damaged, same needs to be renewed.","Miscellaneous","MLC Related","Equipment Related","11.17","Low","","","Vessel received spare Singapore and replaced with new spare. no all found normal","2022-12-23T23:59:35","SCAN220209 - COLD ROOM DOOR GASKET","Completed","2022-12-23T23:59:35","No","No","No","Internal"]
[null,null,null,27655,57508,"45_Fri Nov 11 2022 09:12:24 GMT+0800","2022-10-22T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","BA compressor maintenance log posted near the compressor is torn, same to renew.","LSA / FFA","Safety / LSA / FFA","Human Error","5.15","Medium","","","Vessel carried out renewal of BA triplex cartridge and BA compressor log renewed and posted at location","2022-11-02T23:59:35","","Completed","2022-10-25T23:59:35","No","No","No","Internal"]
[null,null,null,27656,24132,"45_Fri Nov 11 2022 09:16:53 GMT+0800","2022-10-22T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Oil spray was noted below port provision crane. To rectify the leak","Deck - Machinery","ISM Related","Equipment Related","8.5","Very High","","","Vessel carried out inspection of port provision crane. Found one hose with pin hole leak and one in bad shape. Vessel renewed both the hoses and crane tried out. No leaks observed.","2022-11-07T23:59:35","","Completed","2022-10-30T23:59:35","No","No","No","Internal"]
[null,null,null,28472,76993,"45_Mon Jan 16 2023 16:47:34 GMT+0800","2022-10-23T23:59:35","Observation,Defect","Ship Staff","Ship Staff Insp.","ME lube oil purifier oil outlet stop valve malfunctioning","E/R - Purifier","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Oil outlet valve opened up and checked, found diaphragm cracked. Stop valve to be renewed.","2023-08-12T23:59:35","SCAN220258","Completed","2023-07-03T23:59:35","No","No","No","Internal"]
[null,null,null,27653,74153,"45_Mon Nov 14 2022 13:55:38 GMT+0800","2022-10-24T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Stbd windlass brake cylinder found leaking from lower end cover.","Deck - Machinery","Mooring","Equipment Related","9.14","Medium","","","Vessel inspected the shaft for the brake cylinder and found heavy pitting. Vessel has temporarily applied silicone sealant on the shaft. Seals for the lower cover are to be inspected and if required same have to be renewed. Planned renewal during loaded passage.\n05-Feb-2023: Shaft & seals renewed. Leak rectified.","2022-12-23T23:59:35","SCAN225080","Completed","2023-01-29T23:59:35","No","No","No","Internal"]
[null,null,null,27657,42099,"45_Fri Nov 11 2022 09:35:05 GMT+0800","2022-10-24T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Paint store sprinkler pipe found to have salt deposits and choking the sprinkler head","LSA / FFA","Safety / LSA / FFA","Human Error,Inappropriate Procedure,Knowledge Based","5.35","Medium","","","Sprinkler heads disconnected and cleaned. Pipe for sprinkler disconnected and arrangement fabricated for testing with fresh water and air blow of pipe lines.","2022-11-04T23:59:35","","Completed","2022-11-01T23:59:35","No","No","No","Internal"]
[null,null,null,29572,72046,"45_Sun Feb 19 2023 15:32:48 GMT+0800","2022-10-30T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Oily water separator  3rd stage filter housing leaking","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","OWS Third stage filter housing renewed with new one","2023-04-24T23:59:35","SCAN220259","Completed","2023-03-31T23:59:35","No","No","No","Internal"]
[null,null,null,27659,39360,"45_Fri Nov 11 2022 09:45:28 GMT+0800","2022-10-31T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Controller for MW #5 and high/low speed controller for MW #12 found leaking","Deck - Mooring Machinery","Mooring","Equipment Related","9.14","Medium","","","To carry out renewal of seals for both controllers.","2022-11-04T23:59:35","","Completed","2022-11-02T23:59:35","No","No","No","Internal"]
[null,null,null,27660,41442,"45_Fri Nov 11 2022 09:52:57 GMT+0800","2022-11-02T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Ballast overboard valve (BA 040) on main deck found leaking oil","Deck - Pipe / Fittings,Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.80","Medium","","","Manual remote valve disconnected. Found the oil hydraulic oil reservoir badly wasted and corroded. Build up jOb carried out with steel putty. Hydraulic lines found with cordobond. Same to be repaired.","2022-11-05T23:59:35","","Completed","2022-11-04T23:59:35","No","No","No","Internal"]
[null,null,null,27661,42715,"45_Mon Nov 14 2022 13:58:34 GMT+0800","2022-11-04T23:59:35","Observation","Ship Staff","Ship Staff Insp.","VRCS return line near hydraulic box #4 found leaking.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","11.4","Very High","","","Pipe section removed from location. Pipe section renewed flange to flange and tried out to normal working pressure. Found in good order while testing.","2022-11-05T23:59:35","","Completed","2022-11-05T23:59:35","No","No","No","Internal"]
[null,null,null,27790,63089,"45_Sat Nov 26 2022 08:38:52 GMT+0800","2022-11-11T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Valve BA 025 (Ballast Eductor suction - Port side) found to be not opening completely.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","Valve checked at location with manual pump. Found not operating. Actuator dismantled and tried out. Found operating normally with hand pump. Valve removed from location and  dismantled. Found spindle end grinded and not smooth and round. Spindle rounded near socket and tried out. Found opening normal. Valve timing adjusted.","2022-11-18T23:59:35","","Completed","2022-11-17T23:59:35","No","No","No","Internal"]
[null,null,null,27789,63281,"45_Sat Nov 26 2022 08:42:22 GMT+0800","2022-11-13T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Pipe sections found thinned down on MW#7 - Delivery & return line","Deck - Machinery,Deck - Mooring Machinery","Mooring","Equipment Related","9.14","Medium","","","Pipe section removed for renewal. Entire pipe lengths renewed and fixed back at location.","2022-11-26T23:59:35","","Completed","2022-11-20T23:59:35","No","No","No","Internal"]
[null,null,null,27791,72654,"45_Sat Nov 26 2022 08:44:06 GMT+0800","2022-11-13T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Hydraulic delivery line for MW#5 found thinned down and needs to be renewed.","Deck - Machinery,Deck - Mooring Machinery","Mooring","Equipment Related","9.14","Medium","","","Pipe section removed for renewal. Pie renewed and fixed back at location after 2 coats of primer & final coat paint. Pipe section tried out under pressure and found no leaks.","2022-11-25T23:59:35","","Completed","2022-11-22T23:59:35","No","No","No","Internal"]
[null,null,null,27788,25544,"45_Sat Nov 26 2022 08:47:39 GMT+0800","2022-11-17T23:59:35","Observation","Ship Staff","Ship Staff Insp.","BWTS filter No.2 drain pipe found with pin hole leak near flange weld.","Cargo Mach.,Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.8","Medium","","","Pipe section removed and the weld seam chipped. Flange welded back to the pipe with new weld. Pipe section wire brushed and painted before fixing at location.","2022-11-21T23:59:35","","Completed","2022-11-20T23:59:35","No","No","No","Internal"]
[null,null,null,27792,40157,"45_Sat Nov 26 2022 12:07:04 GMT+0800","2022-11-17T23:59:35","Observation","Ship Staff","Ship Staff Insp.","4 Pipe sections on VRCS line found to be thinned down and need to be renewed.","Cargo Mach.,Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","","","","","Pipe sections removed and renewed flange to flange. Pipelines coated with 2 coats of primer and final coat paint. ","2022-11-26T23:59:35","","Completed","2022-11-24T23:59:35","No","No","No","Internal"]
[null,null,null,27980,40024,"45_Fri Dec 16 2022 19:43:38 GMT+0800","2022-11-28T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Fresh water generator no:2 condenser cooling water outlet found leaking from weld joint of pressure gauge ,temperature gauge and from seam weld of pipe.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Fresh water generator isolated,pipe dismantled taken to workshop.Pipe welded fitted back in place and tried out.","2022-12-23T23:59:35","","Completed","2022-11-29T23:59:35","No","No","No","Internal"]
[null,null,null,29579,71635,"45_Sun Feb 26 2023 16:42:32 GMT+0800","2022-12-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Main engine and Auxiliary engine mixing  column auto air vent valve leaking.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Both fuel oil mixing column auto vent valves to be overhauled or replaced. Same removed and overhauled. working good.","2023-09-03T23:59:35","","Completed","2023-09-03T23:59:35","No","No","No","Internal"]
[null,null,null,27979,81187,"45_Fri Dec 16 2022 19:49:17 GMT+0800","2022-12-03T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","Fresh water to deck isolation valve from engine room spindle found broken.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Valve renewed.","2022-12-13T23:59:35","","Completed","2022-12-04T23:59:35","No","No","No","Internal"]
[null,null,null,29580,14904,"45_Sun Feb 26 2023 16:45:28 GMT+0800","2022-12-03T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Main engine Unit No.2 Fuel oil pump VIT rack stuck.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Rack to be eased up or fuel pump to be renewed. All fuel pumps and spare overhauled in DD. Working satisfactory.","2023-08-29T23:59:35","","Completed","2023-09-03T23:59:35","No","No","No","Internal"]
[null,null,null,28462,15600,"45_Tue Jan 03 2023 22:17:46 GMT+0800","2022-12-20T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","All 4 cranes de-rusting and painting.","Deck - Machinery","General Appearance","External Factors","11.4","Very High","","","To derust & paint, vessel awaiting suitable anchorage to carry out the aloft job. Job completed in DD.","2023-09-03T23:59:35","","Completed","2023-09-03T23:59:35","No","No","No","Internal"]
[null,null,null,28465,28209,"45_Tue Jan 03 2023 22:30:28 GMT+0800","2022-12-20T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","All Top bracing are not at similar marking. To check with manual and adjusting needs to be done.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Top bracing adjusted as per manual instruction","2023-02-07T23:59:35","","Completed",null,"No","No","No","Internal"]
[null,null,null,28466,78538,"45_Sun Jan 15 2023 14:39:12 GMT+0800","2022-12-20T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Port pumproom blower is operational, however making abnormal noise when in use.","Miscellaneous","Safety / LSA / FFA","Equipment Related","5.18","High","",""," As per history, claw coupling of motor was renewed to resolve the issue. To investigate further.\nOn further investigation, observed motor guard loose making abnormal noise.  Guard tightened up & packing applied between the guard & motor. Noise level observed normal.","2023-02-21T23:59:35","","Completed","2023-03-19T23:59:35","No","No","No","Internal"]
[null,null,null,28468,35403,"45_Sun Jan 15 2023 13:50:28 GMT+0800","2022-12-20T23:59:35","Observation","Ship Staff","Ship Staff Insp.","BWTS - During deballasting, Interlock between valves BA27, BA28 & BA38 is observed to be not functional. This leads to shut down of process few minutes after deballasting is commenced. ","Miscellaneous","Cargo / Ballast Systems","Equipment Related","8.11","Medium","","","At present these valves are operated on manual mode to continue the deballasting process without any interruption. To investigate further.\nTroubleshooting guide received from the maker on 17th April 2023.\n24-Apr-2023: Trouble shooting carried out as per maker's instructions. Interlock working normally.","2023-05-10T23:59:35","","Completed","2023-04-20T23:59:35","No","No","No","Internal"]
[null,null,null,28475,72206,"45_Sun Jan 15 2023 13:42:16 GMT+0800","2022-12-20T23:59:35","Defect","Ship Staff","Ship Staff Insp.","BWTS - Flow control valve is not operational on AUTO mode. Neither it is operational on Manual 'Remote' or 'Local' mode. Valve is controlled by a portable hand pump connected to it.","Miscellaneous","Cargo / Ballast Systems","Equipment Related","8.11","Medium","","","Valve operated several time on auto & manual mode. However, only possible way of operating at present is using portable hand pump. GC raised.\n13-Apr-2023: Checked & rectified by ETO. Cables checked for loose connection & valve operation tried out following trouble shooting. \nAfter trouble shooting valve was operated in both manual & auto mode satisfactorily in static condition (Without any ballasting operation). However, after few minutes of ballast operations at Tanjung Bruas on 26th April 2023, FCV-1211 malfunctioned again & it is being operated using PHP. Trouble shooting is in progress.\n13-May-2023: Trouble shooting carried out again as per maker’s instructions. Observed valve operating satisfactorily.","2023-04-24T23:59:35","","Completed","2023-05-09T23:59:35","No","No","No","Internal"]
[null,null,null,28477,35188,"45_Tue Jan 03 2023 20:32:45 GMT+0800","2022-12-20T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Container found below the port boiler burner control valve to contain oil leak. Oil leakage to rectify","E/R - Aux. Mach.,E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","same leak has been rectified and monitoring.","2023-01-04T23:59:35","","Completed","2022-12-23T23:59:35","No","No","No","Internal"]
[null,null,null,28478,41873,"45_Tue Jan 03 2023 22:26:43 GMT+0800","2022-12-20T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ME Fuel oil heater steam line leakage to rectify","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","ME fuel oil heating end cover all bolts been tighten and leak has been rectified ","2023-01-09T23:59:35","","Completed","2022-12-22T23:59:35","No","No","No","Internal"]
[null,null,null,28479,78786,"45_Tue Jan 03 2023 20:26:29 GMT+0800","2022-12-20T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Work shop fan damper on incinerator tank platform is sluggish. To ease up and test.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","same has been eased up and made it operaional","2022-12-28T23:59:35","","Completed",null,"No","No","No","Internal"]
[null,null,null,28480,26775,"45_Tue Jan 03 2023 22:08:17 GMT+0800","2022-12-20T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Various leaks from the connections of both FWG","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","All leaks rectified.","2023-01-04T23:59:35","","Completed","2023-01-04T23:59:35","No","No","No","Internal"]
[null,null,null,28483,50416,"45_Tue Jan 03 2023 22:33:09 GMT+0800","2022-12-20T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Misc tanks reading indication in CCR having error","Miscellaneous","Cargo / Ballast Systems","Equipment Related","8.1","Very High","","","Tanks level range adjusted as per sounding table to show correct bar height.","2023-01-04T23:59:35","","Completed","2022-12-24T23:59:35","No","No","No","Internal"]
[null,null,null,28484,15887,"45_Tue Jan 03 2023 22:22:00 GMT+0800","2022-12-20T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","No 2 LT cooler SW inlet outlet pipe was having various small SW leaks. To identify and rectify.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","No 2 LT cooler SW inlet outlet pipe was having various small SW leaks. All salt formation on outlet line of LT cooler has been cleaned and leak has been rectified","2023-01-20T23:59:35","","Completed","2022-12-27T23:59:35","No","No","No","Internal"]
[null,null,null,28485,97133,"45_Tue Jan 03 2023 20:38:08 GMT+0800","2022-12-20T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Paint has peeled off from the Sludge holding tank bulkhead in engine room near stbd boiler . High temp paint to apply.","Miscellaneous","General Appearance","Equipment Related","10.32","Very High","","","old paint has been removed , and applied first coat of  primer and then white paint on bulkhead.","2023-01-20T23:59:35","","Completed","2022-12-28T23:59:35","No","No","No","Internal"]
[null,null,null,28486,32574,"45_Tue Jan 03 2023 20:43:47 GMT+0800","2022-12-20T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Vapour line of FWG to repair by hotwork","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Hotwork  been carried out on FWG NO 1 shell pipe and leak has been rectified","2023-01-04T23:59:35","","Completed","2023-01-04T23:59:35","No","No","No","Internal"]
[null,null,null,28487,83194,"45_Tue Jan 03 2023 20:23:47 GMT+0800","2022-12-20T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","No 1 IG blower discharge valve not opening in auto, to rectify.","Cargo Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","NO 1 IG blower discharge valve position-er removed, overhauled and assembled. valve operated , now found working in normal condition.","2023-01-06T23:59:35","","Completed","2023-01-02T23:59:35","No","No","No","Internal"]
[null,null,null,28489,50952,"45_Tue Jan 03 2023 22:11:00 GMT+0800","2022-12-20T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Aft FWG one of the press gauge has turned black. To renew.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Pressure gauge renewed with new spare pressure guage","2023-01-04T23:59:35","","Completed","2023-01-04T23:59:35","No","No","No","Internal"]
[null,null,null,28469,61636,"45_Sun Jan 15 2023 13:58:48 GMT+0800","2022-12-24T23:59:35","Defect","Ship Staff","Ship Staff Insp.","5P WBT level rising & lowering during ballasting & deballasting of other tanks. Suspected either of main of stripper valve not holding.","Miscellaneous","Cargo / Ballast Systems","Equipment Related","8.11","Medium","","","Investigation carried out. Main valve BA020 found not holding. Same inspected & found with damaged seat ring. Seat ring renewed & leak rectified.","2023-01-14T23:59:35","","Completed","2023-01-10T23:59:35","No","No","No","Internal"]
[null,null,null,28470,17797,"45_Sun Jan 15 2023 14:09:57 GMT+0800","2022-12-24T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Port side no. 3 manifold valve actuator shaft observed with pitting leading to seepage of hydraulic oil from the seal & eventually from the valve indicator","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.11","Medium","","","At present new seal is placed to reduce the outflow of oil & entire actuator is swapped with stbd. side no. 3 manifold valve actuator with stop valves shut to stop the flow of hydraulic oil into actuator. Spares received. To renew spares\n05-Apr-2023: Shaft s & seal renewed. Leak rectified.","2023-04-04T23:59:35","SCAN220262 \nSCAN235002","Completed","2023-03-31T23:59:35","No","No","No","Internal"]
[null,null,null,28474,97021,"45_Sun Jan 15 2023 18:09:38 GMT+0800","2022-12-24T23:59:35","Defect","Ship Staff","Ship Staff Insp.","No.1 ECR Unit cooler pressure switch bellow found leaking.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Pressure switch renewed.","2023-04-24T23:59:35","SCAN230003","Completed","2023-03-25T23:59:35","No","No","No","Internal"]
[null,null,null,28464,30748,"45_Sun Jan 15 2023 14:48:54 GMT+0800","2022-12-27T23:59:35","Observation","Ship Staff","Ship Staff Insp.","M11/12 winch operating platform found wasted at several spots.","Miscellaneous","Mooring","External Factors","11.3","Medium","","","Platform removed for repairs. Repairs carried out & fixed back.","2023-01-23T23:59:35","","Completed","2023-01-11T23:59:35","No","No","No","Internal"]
[null,null,null,28488,99798,"45_Fri Jan 06 2023 13:52:00 GMT+0800","2022-12-28T23:59:35","Defect","Ship Staff","Ship Staff Insp.","NO 2 AHU unit fresh air intake flap was hard to operate , stuck in close position.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Same has been eased up, and lubricated.","2023-01-04T23:59:35","","Completed","2022-12-29T23:59:35","No","No","No","Internal"]
[null,null,null,28467,63768,"45_Sun Jan 15 2023 18:28:47 GMT+0800","2022-12-31T23:59:35","Defect","Ship Staff","Ship Staff Insp.","No.2  Economizer  feed water pump mechanical seal leaking.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Mechanical seal to be renewed.","2023-08-12T23:59:35","SCAN230006","Completed","2023-07-20T23:59:35","No","No","No","Internal"]
[null,null,null,28471,72047,"45_Mon Jan 16 2023 16:38:20 GMT+0800","2023-01-02T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Sewage collecting tank level gauge not working.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Level gauge renewed with spare new one. Presently liquid level indicator is working and in good order.","2023-10-13T23:59:35","SCAN230035","Completed","2023-10-07T23:59:35","No","No","No","Internal"]
[null,null,null,28476,97160,"45_Mon Jan 16 2023 21:21:19 GMT+0800","2023-01-02T23:59:35","Observation","Ship Staff","Ship Staff Insp.","No,2  LT Cooler chemical cleaning valve leaking from body.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Valve renewed","2023-02-06T23:59:35","","Completed",null,"No","No","No","Internal"]
[null,null,null,28481,64657,"45_Sun Jan 15 2023 14:31:45 GMT+0800","2023-01-03T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Pumproom O2 sensor shows irratic reading at intervals. After calibration reading remains stable for few days & again it starts showing erratic reading. ","Miscellaneous","Safety / LSA / FFA","Equipment Related","8.46","Very High","","","Trouble shooting is carried out by ETO. Sensor cleaned & fixed back. At present working satisfactorily.","2023-01-07T23:59:35","","Completed","2023-01-04T23:59:35","No","No","No","Internal"]
[null,null,null,28482,74135,"45_Sun Jan 15 2023 14:23:27 GMT+0800","2023-01-03T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Pumproom entrance I.S. telephone operational for buzzing but can not hear anything on this phone & can not receive any voice from this phone.","Miscellaneous","Safety / LSA / FFA","Equipment Related","5.14","Very High","","","Telephone checked & observed switch not coming up properly on picking up the phone. Switch freed up & communication tested.","2023-01-07T23:59:35","","Completed","2023-01-05T23:59:35","No","No","No","Internal"]
[null,null,null,29575,46904,"45_Mon Feb 20 2023 19:45:55 GMT+0800","2023-01-03T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Pump room gas detection system O2 sensor is showing erratic reading at several occasions.","Miscellaneous","Safety / LSA / FFA","Equipment Related","5.22","High","","","New sensor was received and fitted, same working satisfactory.","2023-06-09T23:59:35","SCAN235020","Completed","2023-05-28T23:59:35","No","No","No","Internal"]
[null,null,null,28463,27831,"45_Sun Jan 15 2023 18:17:36 GMT+0800","2023-01-05T23:59:35","Observation","Ship Staff","Ship Staff Insp.","grey water overboard pipe section has pin holes (leaking)","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","fabricated new pipe sections for grey water overboard line and installed in place.","2023-01-20T23:59:35","","Completed","2023-01-16T23:59:35","No","No","No","Internal"]
[null,null,null,28473,23534,"45_Mon Jan 16 2023 16:35:15 GMT+0800","2023-01-07T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Economizer soot blowers: leaking from both side steam and exhaust side.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Both soot blowers removed during drifting and overhauled. Section pipes renewed. Tried out soot blowers during sailing found working good without any steam or exhaust gas leakages.","2023-10-13T23:59:35","","Completed","2023-10-05T23:59:35","No","No","No","Internal"]
[null,null,null,29583,35250,"45_Sun Mar 19 2023 11:10:57 GMT+0800","2023-01-09T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Both FWG Condenser outlet pipe has thin down and found minor leak from pipe","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Pipe to be renewed. Job carried out at DD. No leaks.","2023-08-12T23:59:35","SCAN230019","Completed","2023-09-03T23:59:35","No","No","No","Internal"]
[null,null,null,28661,31854,"45_Thu Jan 19 2023 13:21:56 GMT+0800","2023-01-11T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Stbd. Pumproom blower mesh damaged from several spots","Miscellaneous","General Appearance","External Factors","5.18","High","","","Mesh renewed","2023-02-07T23:59:35","SCAN230007","Completed","2023-01-30T23:59:35","No","No","No","Internal"]
[null,null,null,28673,46776,"45_Tue Jan 31 2023 10:07:18 GMT+0800","2023-01-12T23:59:35","Observation","Ship Staff","Ship Staff Insp.","High temperature aluminium paint is peeling off from some of the engine room exhaust pipings.","Miscellaneous","Eng. / Strg. Comp.","Industry Issue","10.32","Very High","","","Paint flakes have been removed ","2023-04-24T23:59:35","","Completed",null,"No","No","No","Internal"]
[null,null,null,28662,92925,"45_Sun Jan 29 2023 18:53:28 GMT+0800","2023-01-14T23:59:35","Observation","Ship Staff","Ship Staff Insp.","No.2 Fresh water hydrophore  pump mechanical seal leaking.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Mechanical seal cleaned and put back in use.","2023-02-21T23:59:35","","Completed","2023-02-23T23:59:35","No","No","No","Internal"]
[null,null,null,28675,38331,"45_Mon Jan 30 2023 13:47:17 GMT+0800","2023-01-16T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Waste oil service tank low level alarm faulty","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Fault rectified, issue found with wiring on the level switch.","2023-02-15T23:59:35","","Completed","2023-02-23T23:59:35","No","No","No","Internal"]
[null,null,null,28678,51669,"45_Tue Jan 31 2023 20:53:40 GMT+0800","2023-01-17T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Pin hole observed on EGCS sea water pump discharge line after No.2 EGCS pump discharge valve.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Temporary repair carried out by welding doubler plate on the pipe. Complete pipe has to be renewed in dry dock. Same fabricated new in DD with rubber coating. No leaks.","2023-09-03T23:59:35","","Completed","2023-09-03T23:59:35","No","No","No","Internal"]
[null,null,null,28680,19403,"45_Sun Jan 29 2023 19:02:47 GMT+0800","2023-01-18T23:59:35","Observation","Ship Staff","Ship Staff Insp.","No.2 AE fuel oil heater end cover side steam leak.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","End cover gasket  has been renewed. Heater tested for steam and oil leak, Found no leaks","2023-03-24T23:59:35","","Completed","2023-03-10T23:59:35","No","No","No","Internal"]
[null,null,null,28664,43306,"45_Sun Jan 29 2023 19:17:00 GMT+0800","2023-01-18T23:59:35","Observation","Ship Staff","Ship Staff Insp.","No.2 ME fuel oil heater end cover steam leak.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","End cover gasket has been renewed, heater put in use. found no leak","2023-03-24T23:59:35","","Completed","2023-02-27T23:59:35","No","No","No","Internal"]
[null,null,null,28672,97305,"45_Mon Jan 30 2023 13:27:26 GMT+0800","2023-01-19T23:59:35","Observation,Defect","Ship Staff","Ship Staff Insp.","No.2 ME fuel oil heater steam inlet valve not holding ","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Steam inlet valve renewed with new one.","2023-02-18T23:59:35","","Completed","2023-01-26T23:59:35","No","No","No","Internal"]
[null,null,null,28665,46985,"45_Mon Jan 30 2023 13:30:24 GMT+0800","2023-01-19T23:59:35","Defect","Ship Staff","Ship Staff Insp.","No.2 AE fuel oil heater steam inlet valve not holding ","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Steam inlet valve renewed with new one.","2023-02-18T23:59:35","","Completed","2023-01-26T23:59:35","No","No","No","Internal"]
[null,null,null,28667,21890,"45_Mon Jan 30 2023 13:39:53 GMT+0800","2023-01-19T23:59:35","Defect","Ship Staff","Ship Staff Insp.","No. 1 AE fuel oil supply pump mechanical seal leaking","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Mechanical seal cleaned and put back in use.","2023-03-24T23:59:35","","Completed","2023-03-14T23:59:35","No","No","No","Internal"]
[null,null,null,28674,53141,"45_Tue Jan 31 2023 14:06:25 GMT+0800","2023-01-20T23:59:35","Observation","Ship Staff","Ship Staff Insp.","No. 1 COP discharge valve OP246 (Pneumatic control valve) is not operating on intermediate mode. It is either opening fully or closing fully.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.11","Medium","","","Spare controller unit fitted, calibration carried out, found working satisfactory.","2023-04-14T23:59:35","","Completed","2023-05-12T23:59:35","No","No","No","Internal"]
[null,null,null,28663,27121,"45_Sun Jan 29 2023 18:56:42 GMT+0800","2023-01-20T23:59:35","Observation","Ship Staff","Ship Staff Insp.","COPT's main steam stop valve and all three COPT's individual steam valve gland leaking","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Gland packing nipped off.","2023-03-24T23:59:35","","Completed","2023-03-25T23:59:35","No","No","No","Internal"]
[null,null,null,28670,67948,"45_Tue Jan 31 2023 09:08:54 GMT+0800","2023-01-20T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Both Auxiliary boiler water level controller is operated manually during discharging.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Initialisation of feed water control valve positioner carried out. Performance to be checked during next cargo operations.","2023-03-24T23:59:35","","Completed","2023-03-19T23:59:35","No","No","No","Internal"]
[null,null,null,28671,73127,"45_Tue Jan 31 2023 09:33:53 GMT+0800","2023-01-20T23:59:35","Defect","Ship Staff","Ship Staff Insp.","No. 1 Aux boiler water level indicator DP transmitter steam reference leg line drain valve  leaking.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Valve seat found damaged, same renewed with new one.","2023-02-20T23:59:35","","Completed","2023-02-09T23:59:35","No","No","No","Internal"]
[null,null,null,28677,40081,"45_Tue Jan 31 2023 15:55:39 GMT+0800","2023-01-21T23:59:35","Observation","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","Water Ballast Tanks 1 to 5 wings were fitted with tank dome access and a water sample could only be obtained if the water was above the first platform. For definitive water sample vessel required to open manhole covers that were secured with 26 bolts . ","Hull & Tanks,Documentation","Cargo / Ballast Systems","Industry Issue","2.13","Low","","","All WBTs(1 to 5 wings) sampling ports fabricated.","2023-04-26T23:59:35","SCAN230042","Completed","2023-04-16T23:59:35","No","No","No","External"]
[null,null,null,28679,55191,"45_Wed Feb 01 2023 17:00:18 GMT+0800","2023-01-21T23:59:35","Defect","Ship Staff","Ship Staff Insp.","No.1 Aux boiler emitting black smoke sometimes and observed that FD fan damper is fluctuating.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Initialisation of FD fan damper positioner carried out. Performance to be checked during next cargo operations.","2023-03-24T23:59:35","","Completed","2023-03-19T23:59:35","No","No","No","Internal"]
[null,null,null,28666,98266,"45_Mon Jan 30 2023 13:33:20 GMT+0800","2023-01-21T23:59:35","Defect","Ship Staff","Ship Staff Insp.","No.2 Aux Boiler port side gauge glass leaking","E/R - Pipes/ valves & fittings,E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Gauge glass gasket  and glass has been renewed","2023-03-03T23:59:35","","Completed","2023-03-01T23:59:35","No","No","No","Internal"]
[null,null,null,28668,54096,"45_Mon Jan 30 2023 13:53:41 GMT+0800","2023-01-21T23:59:35","Defect","Ship Staff","Ship Staff Insp.","No.1 Aux. boiler feed water inlet valve after controller, gland leaking","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Feed water valve gland packing  renewed","2023-02-20T23:59:35","","Completed","2023-02-10T23:59:35","No","No","No","Internal"]
[null,null,null,29576,89502,"45_Wed Feb 22 2023 22:30:19 GMT+0800","2023-01-23T23:59:35","Observation","Ship Staff","Ship Staff Insp.","M1 mooring winch speed control valve observed to be leaking.","Deck - Mooring Machinery","Mooring","Equipment Related","9.14","Medium","","","Valve inspected. Observed Valve body slightly corroded from inside leading to damage to O rings. For temporary measure, O rings are renewed & leak is rectified. Requisition raised for spare valve block.","2023-04-24T23:59:35","SCAN230044","Completed","2023-04-28T23:59:35","No","No","No","Internal"]
[null,null,null,29389,82061,"45_Fri Feb 17 2023 12:37:29 GMT+0800","2023-01-26T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Safety locker needs to be arranged properly. Not in good condition.","Miscellaneous","General Appearance","Human Error","5.11","Low","","","Safety locker cleaned & arranged","2023-02-21T23:59:35","","Completed","2023-02-11T23:59:35","No","No","No","Internal"]
[null,null,null,29390,40003,"45_Fri Feb 17 2023 12:43:34 GMT+0800","2023-01-26T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Mast horizontal support pipe iwo Anemometer found wasted. Section needs to be cropped up and renewed.","Navigation - Others","Structural Condn. / WT integrity ","External Factors","11.1","High","","","Wasted pipe section renewed by Hot work. Permanent repair carried out.","2023-04-25T23:59:35","","Completed","2023-03-14T23:59:35","No","No","No","Internal"]
[null,null,null,29391,26388,"45_Fri Feb 17 2023 13:20:46 GMT+0800","2023-01-26T23:59:35","Non Conformity","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Main Engine was under FWE command but still found Main Starting air valve in OPEN condition after several hours in port.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Limit switch 120 on starting air valve adjusted.","2023-02-22T23:59:35","","Completed","2023-02-19T23:59:35","No","No","No","Internal"]
[null,null,null,29392,35665,"45_Fri Feb 17 2023 13:25:02 GMT+0800","2023-01-26T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Provision cranes external limit switch blocks are in bad condition. Needs immediate attention.","Deck - Machinery","General Appearance","Equipment Related","11.6","Medium","","","Limit switch blocks derusted & painted.","2023-01-26T23:59:35","","Completed","2023-02-25T23:59:35","No","No","No","Internal"]
[null,null,null,29393,91192,"45_Fri Feb 17 2023 13:29:34 GMT+0800","2023-01-26T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Several Ballast tank man hole covers found rusted and lifting handles found damaged. This needs your immediate attention.","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.6","Medium","","","Ballast tanks man hole covers de-rusting & painting carried out.","2023-04-25T23:59:35","","Completed","2023-04-03T23:59:35","No","No","No","Internal"]
[null,null,null,29394,77360,"45_Fri Feb 17 2023 14:09:22 GMT+0800","2023-01-26T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Ballast tank sounding pipes found rusted.","Deck - Machinery","General Appearance","External Factors","11.4","Very High","","","De rusting and painting carried out.","2023-03-24T23:59:35","","Completed","2023-03-13T23:59:35","No","No","No","Internal"]
[null,null,null,29395,13849,"45_Fri Feb 17 2023 13:26:50 GMT+0800","2023-01-26T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Scupper plug on Starboard boat deck found cemented.","Deck - Pipe / Fittings","General Appearance","Equipment Related","6.20","Medium","","","Cement removed. Condition of scupper checked. Same installed back & integrity test carried out with water. Found holding satisfactorily.","2023-02-21T23:59:35","","Completed","2023-02-06T23:59:35","No","No","No","Internal"]
[null,null,null,29396,59408,"45_Fri Feb 17 2023 14:16:15 GMT+0800","2023-01-26T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Mooring winch brake band limiting screw at the bottom of the band was found flushed with the band. There should always be some gap between the screw and the band. Refer to manual and ensure all are within acceptable limits as per makers.","Deck - Mooring Machinery","Mooring","Equipment Related","9.10","Medium","","","Freeing & adjustment of stopper bolts completed","2023-03-08T23:59:35","","Completed","2023-02-25T23:59:35","No","No","No","Internal"]
[null,null,null,29397,15927,"45_Fri Feb 17 2023 14:23:35 GMT+0800","2023-01-26T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Bosun store davits hook locking plate found jammed.","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.15","Low","","","Davit hook freed up & greased.","2023-02-21T23:59:35","","Completed","2023-02-11T23:59:35","No","No","No","Internal"]
[null,null,null,29398,54224,"45_Fri Feb 17 2023 14:29:59 GMT+0800","2023-01-26T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Metal bracket for Wooden sliding fender on the Port Gangway found rusted and deteriorated. New metal bracket needs to be fabricated and installed.","Deck - Machinery","General Appearance","Equipment Related","11.5","Medium","","","Derusting & painting of metal bracket carried out. Bracket reinstalled with painted wooden fender.","2023-02-21T23:59:35","","Completed","2023-02-20T23:59:35","No","No","No","Internal"]
[null,null,null,29399,15991,"45_Fri Feb 17 2023 14:38:39 GMT+0800","2023-01-26T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Gland for electrical junction boxes on the bridge wing found damaged.","Elect. Mach. & Equip.","General Appearance","Equipment Related,External Factors","11.16","Low","","","Gland renewed.","2023-03-24T23:59:35","","Completed","2023-02-27T23:59:35","No","No","No","Internal"]
[null,null,null,29400,41085,"45_Fri Feb 17 2023 14:13:23 GMT+0800","2023-01-26T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Mooring winch Brake rendering setting indicators are all set haphazardly. There is no uniformity in the system.","Deck - Machinery","Mooring","Equipment Related","9.10","Medium","","","Indicators adjusted as per brake rendering capacity. ","2023-03-24T23:59:35","","Completed","2023-03-13T23:59:35","No","No","No","Internal"]
[null,null,null,29404,99331,"45_Fri Feb 17 2023 14:26:51 GMT+0800","2023-01-26T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Bosun store davit wire needs greasing. Wire was found dry.","Deck - Machinery","General Appearance","Equipment Related","11.15","Low","","","Wire greased.","2023-02-21T23:59:35","","Completed","2023-02-11T23:59:35","No","No","No","Internal"]
[null,null,null,29405,55614,"45_Fri Feb 17 2023 21:52:25 GMT+0800","2023-01-26T23:59:35","Observation,Defect","Ship Staff","Ship Staff Insp.","Pumps and fans are not tripping on MSB upon activating the Emergency stop ESA & ESB push buttons and when CO2 cabinet is opened..","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.8","Medium","","","Timer 5ET in MSB renewed with new one, working satisfactory now.","2023-03-24T23:59:35","","Completed","2023-03-18T23:59:35","No","No","No","Internal"]
[null,null,null,29408,96449,"45_Fri Feb 17 2023 13:10:12 GMT+0800","2023-01-26T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ME cylinder head hydraulic jack stand – Spacers needs to be stacked properly.","E/R - Main Engine","General Appearance","Human Error","10.32","Very High","","","ME cylinder head hydraulic jack stand all spacer adjusted properly and  stacked accordingly","2023-02-10T23:59:35","","Completed","2023-02-07T23:59:35","No","No","No","Internal"]
[null,null,null,29409,61750,"45_Fri Feb 17 2023 13:15:02 GMT+0800","2023-01-26T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ME Cylinder Oil daily tank level glass found gagged.","Hull & Tanks","Eng. / Strg. Comp.","Human Error","10.32","Very High","","","ME Cylinder Oil daily tank level gauge gagging has been  removed and put a  notice only to be use while checking sounding","2023-02-03T23:59:35","","Completed","2023-01-27T23:59:35","No","No","No","Internal"]
[null,null,null,29410,87178,"45_Fri Feb 17 2023 14:32:56 GMT+0800","2023-01-26T23:59:35","Non Conformity","Owner / Marine / Tech. Suptd.","Suptd. Insp.","During LO bunkering no Wilden pump was rigged as part of SOPEP equipment.","Miscellaneous","MARPOL Related","Human Error","6.3","Low","","","Immediately wilden pump rigged up and secured in place","2023-04-25T23:59:35","","Completed","2023-01-26T23:59:35","No","No","No","Internal"]
[null,null,null,29411,90437,"45_Fri Feb 17 2023 13:18:04 GMT+0800","2023-01-26T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","The engine room hard copy filing system (salmon files) is not as per SMS. Get this corrected for ECR and CE office.","Documentation","Cert. & Docu.","Human Error","2.3","High","","","All files are kept in CE office as per SMS control of documented information.","2023-02-21T23:59:35","","Completed","2023-01-27T23:59:35","No","No","No","Internal"]
[null,null,null,29412,98121,"45_Fri Feb 17 2023 13:07:22 GMT+0800","2023-01-26T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Emergency Diesel generator room sound powered telephone light found not working","Miscellaneous,Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","Emergency generator room sound powered telephone light replace and checked, now found working","2023-02-10T23:59:35","","Completed","2023-02-03T23:59:35","No","No","No","Internal"]
[null,null,null,29413,45402,"45_Fri Feb 17 2023 12:41:27 GMT+0800","2023-01-26T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Elevator escape hatch dogs on the bridge wing was found jammed. This is an emergency escape and needs to be free at all times.","Miscellaneous","Safety / LSA / FFA","Equipment Related","5.11","Low","","","Elevator escape hatch dogs on the bridge eased up and made free.","2023-02-21T23:59:35","","Completed","2023-02-11T23:59:35","No","No","No","Internal"]
[null,null,null,29414,33652,"45_Fri Feb 17 2023 13:03:47 GMT+0800","2023-01-26T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Emergency Diesel Generator LSMGO in use Lab analysis sample is dated 21 October 2015. In 7.3 years it is expected that the above LSMGO has been consumed.","Documentation","Eng. / Strg. Comp.","External Factors","2.3","High","","","Latest analysis report posted in place.","2023-02-21T23:59:35","","Completed","2023-01-30T23:59:35","No","No","No","Internal"]
[null,null,null,29574,46042,"45_Mon Feb 20 2023 19:43:47 GMT+0800","2023-01-27T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Echo sounder slave display unit in bridge overhead panel shows very faint display at night from conning position.","Navigation - Echo Sounder / Speed Log","Navigation","Equipment Related","4.7","High","","","New received echo sounder slave display fitted on the bridge overhead panel, working satisfactory.","2023-06-26T23:59:35","","Completed","2023-06-06T23:59:35","No","No","No","Internal"]
[null,null,null,30408,53426,"45_Thu Jun 15 2023 16:48:46 GMT+0800","2023-01-29T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","The engine room hard copy filing system (salmon files) is not as per SMS. Get this corrected for ECR and CE office.","Documentation","Cert. & Docu.","Behaviour Based,Human Error,Knowledge Based","10.1","Medium","","","Files to be made as per sms requirements","2023-06-26T23:59:35","","Completed","2023-06-09T23:59:35","No","No","No","Internal"]
[null,null,null,30409,13947,"45_Thu Jun 15 2023 16:57:53 GMT+0800","2023-01-29T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Emergency Diesel Generator LSMGO in use Lab analysis sample is dated 21 October 2015. In 7.3 years it is expected that the above LSMGO has been consumed","Miscellaneous","Emgcy. Systems","Human Error,Industry Issue,Behaviour Based","10.35","Very High","","","Latest lab analysis report to be posted","2023-06-26T23:59:35","","Completed","2023-06-12T23:59:35","No","No","No","Internal"]
[null,null,null,30410,30796,"45_Thu Jun 15 2023 16:51:48 GMT+0800","2023-01-29T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ME cylinder head hydraulic jack stand – Spacers needs to be stacked properly.","Miscellaneous","Eng. / Strg. Comp.","Behaviour Based","","","","","Spacres shifted to original box above ecr","2023-06-26T23:59:35","","Completed","2023-06-16T23:59:35","No","No","No","Internal"]
[null,null,null,30418,25682,"45_Thu Jun 15 2023 16:46:13 GMT+0800","2023-01-29T23:59:35","Non Conformity","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Main Engine was under FWE command but still found Main Starting air valve in OPEN condition after several hours in port.","E/R - Main Engine","Eng. / Strg. Comp.","Human Error","10.1","Medium","","","ME start air valve shut.","2023-04-28T23:59:35","","Completed","2023-02-26T23:59:35","No","No","No","Internal"]
[null,null,null,30419,21971,"45_Thu Jun 15 2023 16:50:48 GMT+0800","2023-01-29T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ME Cylinder Oil daily tank level glass found gagged.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Human Error","10.17","Very High","","","Gagging device removed from place.\n","2023-04-28T23:59:35","","Completed","2023-01-29T23:59:35","No","No","No","Internal"]
[null,null,null,30420,70526,"45_Thu Jun 15 2023 16:56:11 GMT+0800","2023-01-29T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","EDG room sound powered telephone light found not working","Elect. Mach. & Equip.","Emgcy. Systems","Human Error,Knowledge Based,Industry Issue","10.32","Very High","","","Light made functional","2023-04-28T23:59:35","","Completed","2023-02-04T23:59:35","No","No","No","Internal"]
[null,null,null,30421,91587,"45_Thu Jun 15 2023 17:01:24 GMT+0800","2023-01-29T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Gland for electrical junction boxes on the bridge wing found damaged.","Elect. Mach. & Equip.","Safety / LSA / FFA","External Factors,Equipment Related,Industry Issue","10.37","Medium","","","Gland renewed.","2023-04-28T23:59:35","","Completed","2023-02-02T23:59:35","No","No","No","Internal"]
[null,null,null,30422,15018,"45_Thu Jun 15 2023 17:06:53 GMT+0800","2023-01-29T23:59:35","Non Conformity","Owner / Marine / Tech. Suptd.","Suptd. Insp.","During LO bunkering no Wilden pump was rigged as part of SOPEP equipment.","Miscellaneous","","Behaviour Based,Human Error,Industry Issue,Knowledge Based","","","","","Wilden pump was rigged","2023-04-28T23:59:35","","Completed","2023-01-29T23:59:35","No","No","No","Internal"]
[null,null,null,30427,89445,"45_Thu Jun 15 2023 23:00:02 GMT+0800","2023-01-29T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Safety locker needs to be arranged properly. Not in good condition.","Accommodation","General Appearance","Behaviour Based","11.13","Low","","","Safety locker cleaned & arranged","2023-02-24T23:59:35","","Completed","2023-02-14T23:59:35","No","No","No","Internal"]
[null,null,null,30428,29258,"45_Thu Jun 15 2023 23:02:51 GMT+0800","2023-01-29T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Elevator escape hatch dogs on the bridge wing was found jammed. This is an emergency escape and needs to be free at all times.","Miscellaneous","General Appearance","Equipment Related","11.13","Low","","","Elevator escape hatch & maintenance hatch freed & greased up.","2023-02-24T23:59:35","","Completed","2023-02-14T23:59:35","No","No","No","Internal"]
[null,null,null,30429,17774,"45_Thu Jun 15 2023 23:06:55 GMT+0800","2023-01-29T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Provision cranes external limit switch blocks are in bad condition. Needs immediate attention.","Deck - Machinery","","Equipment Related","11.6","Medium","","","Limit switch blocks derusted & painted.","2023-02-24T23:59:35","","Completed","2023-02-28T23:59:35","No","No","No","Internal"]
[null,null,null,30430,49532,"45_Thu Jun 15 2023 23:08:55 GMT+0800","2023-01-29T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Scupper plug on Starboard boat deck found cemented.","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","Inappropriate Procedure","6.20","Medium","","","Cement removed. Condition of scupper checked. Same installed back & integrity test carried out with water. Found holding satisfactorily.","2023-02-24T23:59:35","","Completed","2023-02-09T23:59:35","No","No","No","Internal"]
[null,null,null,30431,51972,"45_Thu Jun 15 2023 23:11:15 GMT+0800","2023-01-29T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Several Ballast tank man hole covers found rusted and lifting handles found damaged. This needs your immediate attention.","Hull & Tanks","Structural Condn. / WT integrity ","Equipment Related","11.6","Medium","","","Derusting & painting carried out.","2023-04-28T23:59:35","","Completed","2023-04-04T23:59:35","No","No","No","Internal"]
[null,null,null,30432,81567,"45_Thu Jun 15 2023 23:12:57 GMT+0800","2023-01-29T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Ballast tank sounding pipes found rusted.","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","External Factors","11.4","Very High","","","De rusting and painting carried out.","2023-03-27T23:59:35","","Completed","2023-03-16T23:59:35","No","No","No","Internal"]
[null,null,null,30433,23418,"45_Thu Jun 15 2023 23:14:45 GMT+0800","2023-01-29T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Mooring winch Brake rendering setting indicators are all set haphazardly. There is no uniformity in the system.","Deck - Mooring Machinery","Mooring","Human Error","9.10","Medium","","","Indicators adjusted as per brake rendering capacity","2023-03-27T23:59:35","","Completed","2023-03-16T23:59:35","No","No","No","Internal"]
[null,null,null,30434,52515,"45_Thu Jun 15 2023 23:16:29 GMT+0800","2023-01-29T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Mooring winch brake band limiting screw at the bottom of the band was found flushed with the band. There should always be some gap between the screw and the band. Refer to manual and ensure all are within acceptable limits as per makers.","Deck - Mooring Machinery","Mooring","Human Error","9.10","Medium","","","Freeing & adjustment of stopper bolts completed","2023-02-24T23:59:35","","Completed","2023-02-28T23:59:35","No","No","No","Internal"]
[null,null,null,30435,43651,"45_Thu Jun 15 2023 23:05:19 GMT+0800","2023-01-29T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Mast horizontal support pipe iwo Anemometer found wasted. Section needs to be cropped up and renewed.","Accommodation","General Appearance","External Factors","11.4","Very High","","","Wasted pipe section renewed by Hot work. Permanent repair carried out.","2023-04-28T23:59:35","","Completed","2023-03-17T23:59:35","No","No","No","Internal"]
[null,null,null,30436,20925,"45_Thu Jun 15 2023 23:19:38 GMT+0800","2023-01-29T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Bosun store davit wire needs greasing. Wire was found dry.","Deck - Machinery","General Appearance","Equipment Related","11.15","Low","","","Wire greased","2023-02-24T23:59:35","","Completed","2023-02-14T23:59:35","No","No","No","Internal"]
[null,null,null,30437,67394,"45_Thu Jun 15 2023 23:21:04 GMT+0800","2023-01-29T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Metal bracket for Wooden sliding fender on the Port Gangway found rusted and deteriorated. New metal bracket needs to be fabricated and installed.","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.5","Medium","","","Derusting & painting of bracket carried out. Same secured back.","2023-03-13T23:59:35","","Completed","2023-02-23T23:59:35","No","No","No","Internal"]
[null,null,null,30438,35258,"45_Thu Jun 15 2023 23:18:14 GMT+0800","2023-01-29T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Bosun store davits hook locking plate found jammed.","Deck - Machinery","General Appearance","Equipment Related","11.15","Low","","","Davit hook freed up & greased.","2023-02-24T23:59:35","","Completed","2023-02-14T23:59:35","No","No","No","Internal"]
[null,null,null,29401,31367,"45_Fri Feb 17 2023 21:55:00 GMT+0800","2023-02-03T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Engine room overhead crane low up & low down mode is not operational .","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Up and low mode is operation checked.","2023-02-21T23:59:35","","Completed","2023-02-21T23:59:35","No","No","No","Internal"]
[null,null,null,29406,11324,"45_Fri Feb 17 2023 22:18:33 GMT+0800","2023-02-03T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Emergency fire pump vacuum pump unit clutch lever is broken.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Spare clutch lever has been received. There is no issue with operation readiness of the Emergency Fire pump. Vacuum unit is in good condition. Only the lever needs to be renewed. Will be renewed during upcoming anchorage","2023-04-24T23:59:35","SCAN230054","Completed","2023-05-21T23:59:35","No","No","No","Internal"]
[null,null,null,29589,23824,"45_Sat Feb 25 2023 08:40:11 GMT+0800","2023-02-04T23:59:35","Defect","Ship Staff","Ship Staff Insp.","During pre arrival checks for load port Ras Tanura, one of the UTI (Sr no. G15529) observed showing “NO MESSAGE” error when switched on.","Miscellaneous","Cargo / Ballast Systems","Equipment Related","8.12","Medium","","","On investigation, observed that tape was damaged from the end close to winding unit. Damaged tape was replaced and renewed with  the spare tape onboard keeping the same sensor. After renewal, UTI was tried out & working satisfactorily.  Requisition for new tape raised to keep as a spare (SCAN230045).","2023-02-07T23:59:35","","Completed","2023-02-06T23:59:35","No","No","No","Internal"]
[null,null,null,29403,24548,"45_Fri Feb 17 2023 22:14:58 GMT+0800","2023-02-04T23:59:35","Observation","Ship Staff","Ship Staff Insp.","No. 2 AE turbo charger tachometer digital display unit  faulty.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Wirings checked and tightened.","2023-03-24T23:59:35","","Completed","2023-03-25T23:59:35","No","No","No","Internal"]
[null,null,null,29590,51222,"45_Sun Feb 26 2023 08:02:32 GMT+0800","2023-02-07T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Fresh water line near helicopter deck observed to have pin hole leak.","Deck - Pipe / Fittings","General Appearance","External Factors","11.4","Very High","","","Repairs carried out. Leak rectified.","2023-03-08T23:59:35","","Completed","2023-03-03T23:59:35","No","No","No","Internal"]
[null,null,null,29573,68714,"45_Mon Feb 20 2023 19:39:32 GMT+0800","2023-02-09T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Telegraph logger (printer) self winding drum is not operating at several occasions. At some times it does not allow to wind the paper resulting in overlogging (Overwriting) of the data","Navigation - Others","Navigation","Equipment Related","4.7","High","","","Spare telegraph printer received and replaced with the defective printer.\nNew printer found working satisfactorily.","2023-04-24T23:59:35","SCAN235013","Completed","2023-04-29T23:59:35","No","No","No","Internal"]
[null,null,null,29594,80151,"45_Mon Mar 20 2023 04:25:25 GMT+0800","2023-02-09T23:59:35","Defect","Ship Staff","Nav Audit / Verification","The print out received from Navtex Printer are not clear.","Navigation - GMDSS & Communication","Navigation","Equipment Related","4.7","High","","","Comments received from Superintendent as per mail dated 17 March 2023 Quote \"This DPU-414 is small printer and mechanism is plastic base with thermal printer. It is wear and tear items. We will supply new printer during Singapore call. Vessel can install same. \" Unquote.\nNew Navtex printer received on 23 Mar 2023 and same installed.\n","2023-03-24T23:59:35","","Completed","2023-03-17T23:59:35","No","No","No","Internal"]
[null,null,null,29598,64814,"45_Sat Feb 25 2023 22:57:28 GMT+0800","2023-02-09T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Port side aft Foam monitor - Near break of accommodation found not moving in the vertical sector","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.38","High","","","New foam monitor Turret received at Singapore.\nInstalled on 27 March 2023.","2023-03-24T23:59:35","SCAN220271","Completed","2023-03-20T23:59:35","No","No","No","Internal"]
[null,null,null,29588,48919,"45_Sat Feb 25 2023 22:50:03 GMT+0800","2023-02-10T23:59:35","Defect","Ship Staff","Ship Staff Insp.","M4 mooring winch hydraulic return line found leaking.","Deck - Pipe / Fittings","Mooring","External Factors","9.14","Medium","","","Complete pipe renewed.","2023-02-21T23:59:35","","Completed","2023-02-21T23:59:35","No","No","No","Internal"]
[null,null,null,29593,43355,"45_Tue Mar 14 2023 01:07:19 GMT+0800","2023-02-10T23:59:35","Other","Ship Staff","Ship Staff Insp.","Tank pressure display screen for displaying pressure of individual tanks on bridge to be installed. Vessel has received the display unit under RO SCAN225055.","Miscellaneous","Cargo / Ballast Systems","Equipment Related","","","","","Display installed. Software upgrade carried out on Rosemount PC. Display operational. Individual tank pressure verified with display on Rosemount display in CCR unit.","2023-03-08T23:59:35","","Completed","2023-03-02T23:59:35","No","No","No","Internal"]
[null,null,null,29587,27329,"45_Mon Feb 20 2023 14:10:46 GMT+0800","2023-02-11T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Aft whistle is making low noise when operated.","Navigation - Others","","Equipment Related","4.7","High","","","Air flow checked & cleared up. Noise found normal on trying out.","2023-02-21T23:59:35","","Completed","2023-02-17T23:59:35","No","No","No","Internal"]
[null,null,null,29577,75074,"45_Sat Feb 25 2023 23:00:20 GMT+0800","2023-02-13T23:59:35","Observation","Ship Staff","Ship Staff Insp.","CO2 bottle cabinet on poop deck for emergency generator fixed fire fighting system is badly rusted. CO2 room bottles also showing sign of rust from the bottom","LSA / FFA","Safety / LSA / FFA","External Factors","5.40","Very High","","","Derusting & painting of cabinet carried out. ","2023-02-21T23:59:35","","Completed","2023-03-04T23:59:35","No","No","No","Internal"]
[null,null,null,29578,29269,"45_Sat Feb 25 2023 23:07:47 GMT+0800","2023-02-13T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Fire dampers around accommodation/engine room casing needs cosmetic maintenance and renewal of rubber packings.","Miscellaneous","Safety / LSA / FFA","External Factors","5.35","Medium","","","Completed cosmetic maintenance and renewal of rubber packings on the fire dampers around accommodation and engine room casing.","2023-06-11T23:59:35","","Completed","2023-06-11T23:59:35","No","No","No","Internal"]
[null,null,null,29591,39632,"45_Sat Feb 25 2023 23:10:30 GMT+0800","2023-02-13T23:59:35","Defect,Observation","Ship Staff","Ship Staff Insp.","Steering gear room mushroom vent lid (port side) found badly corroded and hard to move while opening/shutting the vent. ","Miscellaneous","Safety / LSA / FFA","External Factors","5.35","Medium","","","New lid fabricated. Necessary derusting & painting carried out.","2023-03-08T23:59:35","","Completed","2023-03-02T23:59:35","No","No","No","Internal"]
[null,null,null,29595,56520,"45_Sun Feb 26 2023 08:08:15 GMT+0800","2023-02-13T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Ballast eductor drive line found holed in an elbow section near pumproom entrance","Deck - Pipe / Fittings","Cargo / Ballast Systems","External Factors","11.4","Very High","","","Repairs carried out.","2023-02-25T23:59:35","","Completed","2023-02-28T23:59:35","No","No","No","Internal"]
[null,null,null,29592,23920,"45_Sat Feb 25 2023 16:02:07 GMT+0800","2023-02-16T23:59:35","Defect","Ship Staff","Ship Staff Insp.","1P WBT sounding pipe damaged at about 20m from deck plating. The pipe is damaged from 2 sleeve joints which are about 1.5meters apart. Location of damaged section: between fr#95-96 at 3rd stringer.","Hull & Tanks","Structural Condn. / WT integrity ","External Factors","2.9","Medium","","","New pipe installed & clamped to make sounding pipe continuous, as temporary repairs.\nDefect recorded in REFMAN","2023-03-08T23:59:35","","Completed","2023-03-02T23:59:35","No","No","No","Internal"]
[null,null,null,29581,20944,"45_Sun Mar 05 2023 21:52:33 GMT+0800","2023-02-19T23:59:35","Defect,Observation","Ship Staff","Ship Staff Insp.","Expansion tank gauge glass spring loaded valve is leaking.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Valve renewed.","2023-04-01T23:59:35","","Completed",null,"No","No","No","Internal"]
[null,null,null,29582,69648,"45_Tue Mar 07 2023 13:49:17 GMT+0800","2023-02-23T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Air driven pump for TRO drain tank does not operate automatically or manually at several occasions leading to over flow of drain tank content on pump room floor","Miscellaneous","Cargo / Ballast Systems","Equipment Related","8.11","Medium","","","Pump overhauled. Observed air motor clogged with dirt. Air motor gasket found worn out & diaphragm was also observed to be hard. After cleaning, pump is operating with better performance, however, at some occasions it ceases to operate. Spare parts ordered for replacement.\nPresently EU drain tank pump from engine room is replaced with pumproom pump. Spares to be installed in engine room EU drain tank pump.","2023-08-12T23:59:35","SCAN230059","Completed","2023-07-26T23:59:35","No","No","No","Internal"]
[null,null,null,29596,29166,"45_Sun Mar 19 2023 07:18:39 GMT+0800","2023-02-27T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Paint store sprinkler system valve observed not holding after trying out.","LSA / FFA","Safety / LSA / FFA","External Factors","5.40","Very High","","","Valve removed for inspection. Observed pittings on seat. Same overhauled, lapped & fitted back.","2023-03-13T23:59:35","","Completed","2023-03-12T23:59:35","No","No","No","Internal"]
[null,null,null,29599,13698,"45_Sun Mar 19 2023 07:24:18 GMT+0800","2023-03-03T23:59:35","Observation","Ship Staff","Ship Staff Insp.","No. 1 , 2, 3  foam monitor valves observed not holding after trying out.","LSA / FFA","Safety / LSA / FFA","External Factors","5.40","Very High","","","Received new gate valves in Singapore. Leaking valves for No. 1, 2 & 3 foam monitor replaced with the new valves. Pressure testing of the foam line carried out. Foam monitor valve function tested. No leaks observed.","2023-05-21T23:59:35","","Completed","2023-05-23T23:59:35","No","No","No","Internal"]
[null,null,null,29584,63414,"45_Wed Mar 22 2023 18:58:58 GMT+0800","2023-03-08T23:59:35","Defect","Ship Staff","Ship Staff Insp.","No 1 HFO Purifier Heater safety valve is leaking.","E/R - Purifier,E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","VALVE REPLACED WITH BOILER FUEL HEATER SAFETY VALVE , SAFETY VALVE SETTING CHANGED TO 5 BAR.","2023-06-26T23:59:35","SCAN230076","Completed","2023-06-10T23:59:35","No","No","No","Internal"]
[null,null,null,29597,45949,"45_Sat Mar 18 2023 07:40:23 GMT+0800","2023-03-08T23:59:35","Defect","Ship Staff","Ship Staff Insp.","No. 2 BWTS filter drain found leaking from the flange neck of the drain pipe below BWTS filter.","Miscellaneous","Cargo / Ballast Systems","External Factors","8.8","Medium","","","Drain pipe removed for repairs. Installed back after repairs.","2023-03-15T23:59:35","","Completed","2023-03-11T23:59:35","No","No","No","Internal"]
[null,null,null,30323,66391,"45_Tue Jun 06 2023 11:50:19 GMT+0800","2023-03-15T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","SERVICE AIR COMPRESSOR BREAKDOWN","E/R - Aux. Mach.","Eng. / Strg. Comp.","Human Error,Equipment Related","10.32","Very High","","","NEW SPARES RECEIVED, ASSEMBLY IN PROGRESS","2023-06-15T23:59:35","SCAN235017","Completed","2023-06-06T23:59:35","No","No","No","Internal"]
[null,null,null,29585,51236,"45_Tue Mar 28 2023 07:04:07 GMT+0800","2023-03-20T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Stbd. HHC - Hook block spacer plate found wasted while maintenance.","Cargo Mach.","General Appearance","External Factors","8.50","Medium","","","Repairs carried out.","2023-03-30T23:59:35","","Completed","2023-03-25T23:59:35","No","No","No","Internal"]
[null,null,null,29586,98074,"45_Tue Mar 28 2023 07:11:59 GMT+0800","2023-03-20T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Port midship store fwd. facing vent louver found wasted during maintenance.","Miscellaneous","General Appearance","External Factors","11.6","Medium","","","Repair carried out.","2023-03-25T23:59:35","","Completed","2023-03-25T23:59:35","No","No","No","Internal"]
[null,null,null,29752,42701,"45_Thu Apr 20 2023 15:32:27 GMT+0800","2023-03-27T23:59:35","Defect,Observation","Ship Staff","Ship Staff Insp.","No.1 AC Compressor motor pulley is damaged.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Motor pulley to be renewed.","2023-05-26T23:59:35","SCAN230091","Completed","2023-05-21T23:59:35","No","No","No","Internal"]
[null,null,null,29753,72637,"0_Thu Apr 20 2023 15:36:11 GMT+0800","2023-03-27T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Main engine Unit No.1 Fwd fuel injector high pressure pipe is leaking.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","HPP to be renewed or overhauled.","2023-05-26T23:59:35","SCAN230013","Completed","2023-05-23T23:59:35","No","No","No","Internal"]
[null,null,null,29754,36721,"45_Thu Apr 20 2023 15:38:44 GMT+0800","2023-04-03T23:59:35","Defect","Ship Staff","Ship Staff Insp.","No.2 boiler water circulating pump gland packing is leaking.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Gland packing has been renewed","2023-07-03T23:59:35","","Completed","2023-04-23T23:59:35","No","No","No","Internal"]
[null,null,null,29755,91044,"0_Thu Apr 20 2023 15:40:23 GMT+0800","2023-04-03T23:59:35","Defect,Observation","Ship Staff","Ship Staff Insp.","Main engine unit no.6 fuel pump top cover is leaking.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Top cover to be overhauled.","2023-05-26T23:59:35","","Completed","2023-05-14T23:59:35","No","No","No","Internal"]
[null,null,null,29750,87860,"45_Thu Apr 20 2023 11:28:34 GMT+0800","2023-04-08T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Port gangway: One of the sheave has came apart from the gangway channel plate. This sheave plate when in operation is being used for swinging the gangway inboard. at present the sheave plate has wasted/come apart from the top end & is holding only from the bottom end.","Miscellaneous","Safety / LSA / FFA","External Factors","5.47","Medium","","","15-Apr-2023: Damaged plate removed completely for temporary repairs.\n18-Apr-2023: Temporary clamping arrangement with sheave installed. Gangway tried out & found working satisfactorily. Further repairs to be planned as per direction of technical department.\n02-May-2023: Job entered in REFMAN for repairs during DD>\n","2023-05-10T23:59:35","","Completed","2023-04-28T23:59:35","No","No","No","Internal"]
[null,null,null,29751,26632,"45_Thu Apr 20 2023 13:08:42 GMT+0800","2023-04-08T23:59:35","Observation","Ship Staff","Ship Staff Insp.","VECS O2 sensor readings is erratic.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.17","Low","","","Defective sensor renewed with a new sensor, found working satisfactory.","2023-06-26T23:59:35","SCAN230095","Completed","2023-05-12T23:59:35","No","No","No","Internal"]
[null,null,null,30326,17723,"45_Mon May 15 2023 12:49:58 GMT+0800","2023-04-08T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Foam monitor stbd  side near break of accommodation leaking from horizontal bearing area.","LSA / FFA","Safety / LSA / FFA","External Factors","5.38","High","","","O-ring in the horizontal sleeving replaced. Foam monitor tested, no leaks observed.\nInspection of all the foam monitors carried out. No leaks observed.","2023-05-26T23:59:35","","Completed","2023-05-23T23:59:35","No","No","No","Internal"]
[null,null,null,29756,25202,"45_Thu Apr 20 2023 20:42:16 GMT+0800","2023-04-09T23:59:35","Defect","Ship Staff","Ship Staff Insp.","No.2 main air compressor lub. oil flexible hose is broken due to brittleness.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Broken Flexible hose is connected with copper pipe as temporary repair. Hose to be renewed with new one.","2023-05-26T23:59:35","SCAN230089","Completed","2023-05-18T23:59:35","No","No","No","Internal"]
[null,null,null,29757,73798,"45_Thu Apr 20 2023 20:54:42 GMT+0800","2023-04-10T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Distance rings installed on No.2 IG blower at non drive end bearing to be removed.","Cargo Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Distance rings have been removed from the NDE as per makers instruction manual. ","2023-05-10T23:59:35","","Completed","2023-04-19T23:59:35","No","No","No","Internal"]
[null,null,null,30329,74143,"45_Tue Jun 06 2023 12:06:01 GMT+0800","2023-05-06T23:59:35","Defect","Ship Staff","Ship Staff Insp.","OVERSPPED TRIP FOR DG#2 NOT WORKING DUE TO DAMAGED GEAR WHEEL","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","LO PUMP TO BE DISMANTLED TO REPLACE WORM WHEEL DRIVE FOR OVERSPEED TRIP.","2023-08-06T23:59:35","","Completed","2023-06-01T23:59:35","No","No","No","Internal"]
[null,null,null,30320,56269,"45_Tue May 16 2023 20:48:58 GMT+0800","2023-05-12T23:59:35","Observation","Ship Staff","Ship Staff Insp.","During Routine inspection of the Port gangway turntable, observed that the bottom plate was rusted and needs immediate de-rusting and inspection. Plate found not wasted but maintenance needs to be carried out. ","Deck - Pipe / Fittings","General Appearance","Equipment Related","5.47","Medium","","","Turntable was lowered to engine room for renewal of wasted / corroded checkered  plate. Sliding platform hydroblasted, coated with two coats of primer and finish coat. After completion of repair on the turntable same coated with 2 coats of primer and final coat and fitted back in location alongwith the sliding platform. Gangway tested, found working satisfactory.","2023-07-27T23:59:35","","Completed","2023-06-07T23:59:35","No","No","No","Internal"]
[null,null,null,30321,48725,"45_Thu May 18 2023 13:27:46 GMT+0800","2023-05-12T23:59:35","Observation","Ship Staff","Ship Staff Insp.","During Routine inspection of the Starboard gangway turntable, observed that the bottom plate was rusted and needs immediate de-rusting and inspection. Plate found not wasted but maintenance needs to be carried out.","Deck - Pipe / Fittings","General Appearance","Equipment Related","5.47","Medium","","","Starboard side gangway turntable removed and lowered to engine room for hot work repair.  Wasted / corroded checkered plate renewed. Sliding platform removed from location, hydroblasted, close-up inspection carried out, no wastage observed. Same coated with 2 coats of primer and paint same fitted back and tested. ","2023-07-27T23:59:35","","Completed","2023-06-26T23:59:35","No","No","No","Internal"]
[null,null,null,30327,64092,"45_Tue Jun 06 2023 09:40:44 GMT+0800","2023-05-13T23:59:35","Observation","Ship Staff","Ship Staff Insp.","CO2 release cabinet for emergency generator room was found corroded and wasted. Need to fabricate new cabinet.","Deck - Pipe / Fittings","Safety / LSA / FFA","External Factors","5.35","Medium","","","The cabinet was removed and taken to workshop for fabrication. Same fitted back after the repair; applied two coats of primer and finish coat. Emergency operating instructions were stenciled.","2023-06-12T23:59:35","","Completed","2023-05-29T23:59:35","No","No","No","Internal"]
[null,null,null,30322,21208,"45_Mon May 29 2023 15:20:13 GMT+0800","2023-05-14T23:59:35","Defect","Ship Staff","Ship Staff Insp.","BUNKER MANIFOLD STBD SIDE AFT LSMGO LINE VALVE HANDLE BROKEN","Deck - Pipe / Fittings","ISM Related","Equipment Related","8.41","Medium","","","WHEEL REPLACED FROM OLD USED VALVE","2023-08-14T23:59:35","","Completed","2023-05-29T23:59:35","No","No","No","Internal"]
[null,null,null,30411,94232,"45_Thu Jun 15 2023 17:12:46 GMT+0800","2023-05-14T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","MAB - Main Air Bottle no 1 pressure transmitter root valve spindle wheel missing.","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Wheel to be put in place","2023-08-14T23:59:35","","Completed","2023-06-27T23:59:35","No","No","No","Internal"]
[null,null,null,30412,50352,"45_Thu Jun 15 2023 17:18:08 GMT+0800","2023-05-14T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","QCV - Sludge collection tank QCV is not listed in the QCV list. When was this last tried out? QCV to be stenciled on the bulkhead.","Miscellaneous","Eng. / Strg. Comp.","Behaviour Based","","","","","Stenciling to be carried out","2023-06-26T23:59:35","","Completed","2023-06-17T23:59:35","No","No","No","Internal"]
[null,null,null,30413,21311,"45_Thu Jun 15 2023 17:20:42 GMT+0800","2023-05-14T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Pipelines - IG Blower drain line above the IGG found holed at 2 places. Pipe lines needs to be renewed.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.55","Low","","","New pipeline to be fabricated","2023-06-26T23:59:35","","Completed","2023-06-25T23:59:35","No","No","No","Internal"]
[null,null,null,30414,71553,"45_Thu Jun 15 2023 23:49:04 GMT+0800","2023-05-14T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Bosun store - Port side anchor wash line found holed and leaking. Pipeline renewal is required.","Deck - Pipe / Fittings","Safety / LSA / FFA","Equipment Related","11.4","Very High","","","Damaged / cracked globe valve has been replaced for the port side bosun store bilge suction. Pressure testing of the piping system carried out, no leaks observed.","2023-07-13T23:59:35","","Completed","2023-06-06T23:59:35","No","No","No","Internal"]
[null,null,null,30415,82991,"45_Thu Jun 15 2023 23:54:14 GMT+0800","2023-05-14T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Accommodation - There was a mail from HSQE for securing of all gym equipment’s, however no action has been taken yet. All equipment’s to be secured in place. Gym not to be used till this is secured","Accommodation","General Appearance","Inappropriate Procedure","11.13","Low","","","Securing of the heavy weights & equipment carried out to prevent rolling damage. Anti-skid mat placed below the gymnasium equipments.","2023-07-13T23:59:35","","Completed","2023-06-10T23:59:35","No","No","No","Internal"]
[null,null,null,30416,57428,"45_Thu Jun 15 2023 23:45:45 GMT+0800","2023-05-14T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Bridge - Wind alarm Straub light in front of bridge found damaged from base. New base plate to be fabricated","Accommodation","General Appearance","Equipment Related","11.8","Low","","","Base plate power tooled and inspected, found in satisfactory condition. No wastage observed. Same coated with two coats of primer and paint.","2023-07-13T23:59:35","","Completed","2023-06-10T23:59:35","No","No","No","Internal"]
[null,null,null,30417,51894,"45_Thu Jun 15 2023 23:55:39 GMT+0800","2023-05-14T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Deck - Starboard slop steam lines are holed at several locations and needs to be renewed.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.15","High","","","Vessel carried out pressure testing of steam coils for both port & stbd slop tanks. 2 coils leaking inside the tank in Slop Port tank. Steam traps have been holed at various locations. New RO for steam traps have been raised SCAN230131. After departure Singapore, vessel will remove the steam manifolds on deck both the side and carry out hydroblasting and lower the same in engine room workshop for permanent repair.","2023-08-13T23:59:35","","Completed","2023-07-08T23:59:35","No","No","No","Internal"]
[null,null,null,30423,89882,"45_Thu Jun 15 2023 17:10:16 GMT+0800","2023-05-14T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","EDG - CO2 panel for the EDG found very hard to open as the door hinge is broken and needs to be repaired.","LSA / FFA","Safety / LSA / FFA","Equipment Related,Industry Issue","","","","","CO2 panel repaired with new fabricated frame","2023-07-14T23:59:35","","Completed","2023-05-18T23:59:35","No","No","No","Internal"]
[null,null,null,30424,44090,"45_Thu Jun 15 2023 17:13:51 GMT+0800","2023-05-14T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","VRCS -Near the VRCS several chemical drums are kept which were used for filing up of LO in the VRCS system. All chemical drums to be removed. This is a very wrong practice and company is strictly against such practices of using chemical drums to fill up LO.","Miscellaneous","Eng. / Strg. Comp.","Human Error","","","","","Drums removed","2023-05-14T23:59:35","","Completed","2023-05-14T23:59:35","No","No","No","Internal"]
[null,null,null,30425,43775,"45_Thu Jun 15 2023 17:15:20 GMT+0800","2023-05-14T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Boiler valves - Greasing of all valve spindles to be carried out as all of them dry and hard to operate.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related,Knowledge Based","10.32","Very High","","","Boiler valves spindle greased","2023-06-14T23:59:35","","Completed","2023-06-08T23:59:35","No","No","No","Internal"]
[null,null,null,29402,70361,"45_Fri Feb 17 2023 22:11:02 GMT+0800","2023-05-14T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Isolating valve 26V for LT coolers on Main cooling sea water line is stuck in open condition .","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Valve gear mechanism opened and inspected, found in good condition. Suspecting the valve stuck in open position, valve needs to be eased up. Valve replaced in DD. ","2023-08-14T23:59:35","SCAN230123","Completed","2023-09-03T23:59:35","No","No","No","Internal"]
[null,null,null,30426,33582,"45_Thu Jun 15 2023 17:17:11 GMT+0800","2023-05-14T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Electrical - All starter panels ventilation port filters are found heavily choked. Inspection of all such ports to be carried out and cleaned.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","External Factors,Human Error,Industry Issue,Knowledge Based","","","","","","2023-05-28T23:59:35","","Completed","2023-05-28T23:59:35","No","No","No","Internal"]
[null,null,null,30439,43074,"45_Thu Jun 15 2023 23:27:29 GMT+0800","2023-05-14T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Cleaning and removing of all unwanted clothes/helmets and debris to be carried out from both the changing lockers. Many lockers are also filled with garbage and must be kept in cleaning condition.","Accommodation","General Appearance","Behaviour Based","11.13","Low","","","Both the changing locker old boiler suits, safety shoes & helmets removed. Each locker was cleaned by the respective personnel. Routine checks of the same carried out during weekly inspection rounds.","2023-05-21T23:59:35","","Completed","2023-05-23T23:59:35","No","No","No","Internal"]
[null,null,null,30440,15454,"45_Thu Jun 15 2023 23:29:45 GMT+0800","2023-05-14T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Operating procedures in the Fire Control station still bear the name of SAMCO SCANDINAVIA","Miscellaneous","Safety / LSA / FFA","Human Error","5.4","High","","","Same changed to own vessel name. Various places checked and corrected.","2023-05-21T23:59:35","","Completed","2023-05-16T23:59:35","No","No","No","Internal"]
[null,null,null,30441,28846,"45_Thu Jun 15 2023 23:43:07 GMT+0800","2023-05-14T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Bridge - Fire round plan on the bridge has not mention of the rounds to be taken in the EGCS room. New route plan to be made and request send to office for approval.","Miscellaneous","Safety / LSA / FFA","Inappropriate Procedure","4.4","High","","","Received from office approved plan for fire rounds in the EGCS room. A copy of same has been posted on the bridge. Training carried out for the officers & crew incharge for carrying out fire rounds. Fire rounds now taken as per the approved route as mentioned in the plan.","2023-05-21T23:59:35","","Completed","2023-05-16T23:59:35","No","No","No","Internal"]
[null,null,null,30442,64004,"45_Thu Jun 15 2023 23:51:17 GMT+0800","2023-05-14T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Provision store - Make one rack dedicated for 'goods to be expired soon' section.","Accommodation","General Appearance","Inappropriate Procedure","11.13","Low","","","Galley team carried out extensive search for goods to be expiring soon and shifted those items to one dedicated rack in provision store. Same stencilled for \"GOODS TO BE EXPIRED SOON\"","2023-05-29T23:59:35","","Completed","2023-05-21T23:59:35","No","No","No","Internal"]
[null,null,null,30443,98527,"45_Thu Jun 15 2023 23:52:56 GMT+0800","2023-05-14T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Manifold - Starboard side manifold grating is new in condition but it was found sagging at few locations. This could be a major hinderance when reducers are kept. All the gratings need to be aligned to land on the frame.","Deck - Pipe / Fittings","General Appearance","External Factors","6.6","Medium","","","All the manifold gratings on both the side were adjusted / shifted to allow resting on the frame. Same secured with the securing clamps.","2023-06-13T23:59:35","","Completed","2023-05-25T23:59:35","No","No","No","Internal"]
[null,null,null,30444,75985,"45_Thu Jun 15 2023 23:58:18 GMT+0800","2023-05-14T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","EDG - CO2 panel for the EDG found very hard to open as the door hinge is broken and needs to be repaired.","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.35","Medium","","","Emergency Generator CO2 box was removed from location and lowered to engine room workshop for hot work repair, same fitted back after repair. Two coats of primer and final coat applied. Emergency operating instructions were stencilled. ","2023-07-13T23:59:35","","Completed","2023-05-29T23:59:35","No","No","No","Internal"]
[null,null,null,30445,47573,"45_Thu Jun 15 2023 23:38:36 GMT+0800","2023-05-14T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Life boat - Gripes condition is not very good and looks rusted. Need to be de-rusted and greased properly.","LSA / FFA","Safety / LSA / FFA","External Factors","5.28","Very High","","","All the lifeboat gripes were de-rusted and applied with a fresh layer of grease.","2023-05-29T23:59:35","","Completed","2023-05-14T23:59:35","No","No","No","Internal"]
[null,null,null,30446,40478,"45_Thu Jun 15 2023 23:35:52 GMT+0800","2023-05-14T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Pump room - welding burn marks are visible at multiple locations in the PR. All need to be identified and painted.","Hull & Tanks","General Appearance","Inappropriate Procedure","8.44","High","","","Scrapped off the burn marks, 2 coats of finish coat applied.","2023-05-29T23:59:35","","Completed","2023-05-29T23:59:35","No","No","No","Internal"]
[null,null,null,30447,16650,"45_Thu Jun 15 2023 23:32:06 GMT+0800","2023-05-14T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","HHC - New Emergency pump for the HHC is lying in the CCR. This needs to be put in place and checked if all the connections are appropriate for the vessel. Emergency operation testing of the cranes to be tested.","Deck - Machinery","Cargo / Ballast Systems","Equipment Related","8.50","Medium","","","Emergency pump shifted to port side midship store. Same tagged for easy identification. Connections for the same verified & emergency operations tested, found working satisfactory.","2023-06-13T23:59:35","","Completed","2023-06-09T23:59:35","No","No","No","Internal"]
[null,null,null,30324,41274,"45_Tue Jun 06 2023 19:10:25 GMT+0800","2023-05-24T23:59:35","Defect","Ship Staff","Ship Staff Insp.","M/E UNIT#1, #2, #6 ALPHA LUBRICATOR INLET ACCUMULATOR DIAPHGRAM PUNCTURES","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","REQ RAISED TO REPLACE ACCUMULATOR. JOB CARRIED OUT BY SERVICE ENGINEER AT DD.  ALL ACCUMULATORS CHECKED AND REPLACED AS REQUIRED. ","2023-08-24T23:59:35","SCAN230116","Completed","2023-09-03T23:59:35","No","No","No","Internal"]
[null,null,null,30328,98075,"45_Tue Jun 06 2023 09:46:08 GMT+0800","2023-05-29T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Low expansion foam tank liquid level was not visible in the gauge glass.","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.40","Very High","","","Low expansion foam tank liquid level was physically verified; same found normal. Opened the bottom side of the gauge glass, observed the rubber packing was sealing / blocking the bottom opening preventing the foam liquid from entering in the gauge glass. Same rectified and fitted back. Found showing normal level.","2023-06-04T23:59:35","","Completed","2023-05-30T23:59:35","No","No","No","Internal"]
[null,null,null,29407,35175,"45_Fri Feb 17 2023 23:08:52 GMT+0800","2023-05-29T23:59:35","Defect","Ship Staff","Ship Staff Insp.","No. 1 Fresh water generator jacket water outlet valve not holding.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","VALVES ARE HOLDING RECENTLY ON 27.07.23 CARRIED OUT EVAPORATOR CLEANING.","2023-08-29T23:59:35","","Completed","2023-07-25T23:59:35","No","No","No","Internal"]
[null,null,null,30325,55859,"45_Tue Jun 06 2023 19:11:44 GMT+0800","2023-05-30T23:59:35","Defect","Ship Staff","Ship Staff Insp.","PORT & STBD WINDLASS GEAR CASE SEAL LEAKING","Deck - Mooring Machinery","Mooring","Equipment Related","","","","","NEED TO RENEW SEAL. PO RAISED. JOB COMPLETED IN DD.","2023-09-03T23:59:35","SCAN230164","Completed","2023-09-03T23:59:35","No","No","No","Internal"]
[null,null,null,30938,45423,"45_Sun Jul 02 2023 03:27:42 GMT+0800","2023-06-03T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Return line for the aft mooring hydraulic system found leaking.","Deck - Mooring Machinery","Mooring","Equipment Related","9.14","Medium","","","The leaking section removed from location lowered to engine room workshop for repair. After repair, pipe painted with two coats of primer and finish coat and fitted back. Oil topped off in the hydraulic tank. System purged and tested, no leaks observed.","2023-06-16T23:59:35","","Completed","2023-06-08T23:59:35","No","No","No","Internal"]
[null,null,null,30940,98493,"45_Sun Jul 02 2023 03:34:18 GMT+0800","2023-06-03T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Forecastle store port side bilge suction valve found corroded and cracked.","Deck - Pipe / Fittings","Emgcy. Systems","Equipment Related","6.10","Low","","","The damaged valve replaced with a new valve, same painted & sealed. SEAL LOG updated for the seal number.","2023-07-02T23:59:35","","Completed","2023-06-06T23:59:35","No","No","No","Internal"]
[null,null,null,30941,46265,"45_Sun Jul 02 2023 03:41:48 GMT+0800","2023-06-04T23:59:35","Observation","Ship Staff","Ship Staff Insp.","During ballast tank inspection found few ballast tank domes were jammed / seized which required chain block to turn it.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.18","High","","","Carried out maintenance on the seized ballast tank domes. De-rusting & greasing carried out. Tank domes rotated to ease and free the motion. All other tank domes including cargo tank domes greasing carried out.","2023-07-03T23:59:35","","Completed","2023-06-14T23:59:35","No","No","No","Internal"]
[null,null,null,30939,69491,"45_Sun Jul 02 2023 03:47:05 GMT+0800","2023-06-13T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Found pinhole leak on the hydraulic return line of MW4.","Deck - Mooring Machinery","Mooring","Equipment Related","9.14","Medium","","","The leaking section was removed from location & lowered to engine room for repair. New fabricated return line coated with primer & paint, fitted back and tested. No leaks observed.","2023-06-16T23:59:35","","Completed","2023-06-15T23:59:35","No","No","No","Internal"]
[null,null,null,30934,42797,"45_Sat Jul 01 2023 11:17:44 GMT+0800","2023-06-17T23:59:35","Observation","Ship Staff","Ship Staff Insp.","ECR AMS PANEL ROS2 COMPUTER NOT WORKING NO DISPLAY","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related,Industry Issue","10.32","Very High","","","NEED TO REPLACE CPU AS PER MAKER'S ADVISE. PO RAISED.  SAME REPLACED.","2023-09-17T23:59:35","SCAN235034","Completed","2023-09-03T23:59:35","No","No","No","Internal"]
[null,null,null,30935,42953,"45_Sun Jul 02 2023 03:05:49 GMT+0800","2023-06-21T23:59:35","Observation","Ship Staff","Ship Staff Insp.","During cargo discharging operation, observed the cargo eductor suction gauge in CCR showing erratic reading.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.8","Medium","","","Cargo Eductor Gauge in pump-room inspected, Tubing found to be choked. Same blown and cleared - Working Satisfactory.","2023-07-20T23:59:35","","Completed","2023-07-19T23:59:35","No","No","No","Internal"]
[null,null,null,30936,85462,"45_Sun Jul 02 2023 09:15:22 GMT+0800","2023-06-21T23:59:35","Observation","Ship Staff","Ship Staff Insp.","GE LOPX DISPLAY NOT WORKING","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","NEW DISPLAY TO BE INSTALLED","2023-09-21T23:59:35","SCAN220256","Completed","2023-07-03T23:59:35","No","No","No","Internal"]
[null,null,null,30942,46089,"45_Sun Jul 02 2023 09:18:16 GMT+0800","2023-06-21T23:59:35","Observation","Ship Staff","Ship Staff Insp.","STBD LIFEBOAT RUDDER WAS TESTED HARD OVER PORT  AND STBD. HARD OVER PORT WAS ABOUT HALF THAT OF  WHEN THE RUDDER WAS PUT HARD OVER STBD","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.29","High","","","STEERING ARRANGEMENT DISMANTLED AND FOUND LOCKING SLEEVE LOOSE SAME REPLACED WITH NEW SLEEVE AND LOCKED IN PLACE","2023-09-21T23:59:35","","Completed","2023-06-21T23:59:35","No","No","No","Internal"]
[null,null,null,30937,17359,"45_Sun Jul 02 2023 03:15:23 GMT+0800","2023-06-27T23:59:35","Defect","Ship Staff","Ship Staff Insp.","During ballast water exchange; FCV - 1211 gave failure alarm. Tried operating valve from CCR panel remotely - Not operational. Tried operating with hand pump locally in pumproom - Found operational. Presently Ballast Water Exchange in progress, will reset the error after completion of exchange.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","6.21","High","","","Old history of recurrent fault / error on the FCV-1211, due to vibrations on the valve. Carried out reset as per maker's instructions, alarm reset & valve operation back to normal. Same tested from CCR BWTS panel - Operational.","2023-07-26T23:59:35","","Completed","2023-06-28T23:59:35","No","No","No","Internal"]
[null,null,null,31854,35923,"45_Tue Jul 25 2023 13:37:29 GMT+0800","2023-07-18T23:59:35","Defect","Ship Staff","Ship Staff Insp.","EGCS PAH SENSOR VALUE IS ZERO.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Calibration done by shore technician. ","2023-10-18T23:59:35","","Completed","2023-09-13T23:59:35","No","No","No","Internal"]
[null,null,null,31853,10739,"45_Sun Jul 30 2023 03:44:25 GMT+0800","2023-07-22T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","#1 Main air compressor LP side conrod broken and crankshaft damaged due to seized big end bearing.","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Vessel has no more Hatlappa compressor onboard since vessel is equipped with 2 Nos sperre air compressor.","2023-11-30T23:59:35","SCAN230197","Completed","2023-11-22T23:59:35","No","No","No","Internal"]
[null,null,null,32125,33010,"45_Sun Oct 01 2023 17:06:08 GMT+0800","2023-08-26T23:59:35","Defect","Ship Staff","Ship Staff Insp.","During the Inspection of Cargo Sea-chest valves in pump-room, It was noticed that OP-276 Cargo sea line isolation valve is leaking.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.11","Medium","","","OP-276 Valve dismantled and inspected. One big Rag piece found stuck in the Valve stem and Seat-ring found damaged. Valve was cleaned, rag piece removed, seat-ring renewed and Valve boxed back.","2023-09-29T23:59:35","","Completed","2023-09-28T23:59:35","No","No","No","Internal"]
[null,null,null,32116,62868,"45_Sun Oct 01 2023 16:32:24 GMT+0800","2023-09-10T23:59:35","Observation","Ship Staff","Ship Staff Insp.","No.1 TRO Unit in pump-room is showing Configuration Error. Same to be consulted with the Makers and trouble-shooting to be carried out as per the instructions.","Miscellaneous","Cargo / Ballast Systems","Equipment Related","6.21","High","","","As per the Makers advise, TRO units were powered off / On; After Re-starting configuration error is gone. System priming carried out - Found working Satisfactory. System Put in Use during the Loading operations at Basrah from 04-06 Oct 2023, All found working Satisfactory.","2023-10-02T23:59:35","","Completed","2023-10-06T23:59:35","No","No","No","Internal"]
[null,null,null,32115,19146,"45_Sun Oct 01 2023 16:37:08 GMT+0800","2023-09-11T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","Level Switch (LS1111) for the Electrolyser Discharge side found faulty during the BWE operations. Same is by-passed and operation carried out. Further assessment to be made for rectification or ordering the New one as advised by the makers.","Miscellaneous","Cargo / Ballast Systems","Equipment Related","6.21","High","","","Level switch renewed with spare new one received. Presently working in good order.","2023-12-15T23:59:35","","Completed","2023-12-01T23:59:35","No","No","No","Internal"]
[null,null,null,32113,79468,"45_Sun Oct 01 2023 16:26:34 GMT+0800","2023-09-13T23:59:35","Critical Equipment","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Foam monitor No.5 at manifold area was found leaking during inspection","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.40","Very High","","","Foam monitor No.5 tested to check the leakage, foam monitor found leaking from nozzle and body. After flushing the Monitor, Allen bolts of the body were tightened, leak stopped. Also Valve lip seal packing cleaned, Valve closed properly. No Leaks observed. Smooth operation of valve verified.","2023-10-14T23:59:35","","Completed","2023-09-20T23:59:35","No","No","No","Internal"]
[null,null,null,32117,72708,"45_Sun Oct 01 2023 16:24:07 GMT+0800","2023-09-13T23:59:35","Critical Equipment","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Isolation valve in foam room reported to be leaking. To leap and rectify.\t\t","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.38","High","","","Isolation Valve Dismantled. It was found that seat is not sitting properly due the rust formation in the Guiding channel body. Lip Seal cleaned, Internal surfaces buffed and cleaned. Guiding channel body & Disc body cleaned properly and boxed back. Greasing carried out. Isolation Valve tested - No leakage and smooth operation verified.","2023-10-03T23:59:35","","Completed","2023-09-19T23:59:35","No","No","No","Internal"]
[null,null,null,32123,60242,"45_Sun Oct 01 2023 15:40:17 GMT+0800","2023-09-13T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Boiler water salinity indicator showing high value. To trouble shoot and rectify.\t","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Both Boilers blow down carried out. Presently the chloride content is as follows Boiler#1 - 30PPM, Boiler#2- 30PPM, Cooling water- 20 PPM, Condensate- 10PPM.","2023-09-29T23:59:35","","Completed","2023-09-23T23:59:35","No","No","No","Internal"]
[null,null,null,32124,90010,"45_Sun Oct 01 2023 15:42:31 GMT+0800","2023-09-13T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","In Engine room EGCS renewed pipe section to paint.\t","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","EGCS renewed pipe section painted.","2023-09-23T23:59:35","","Completed","2023-09-17T23:59:35","No","No","No","Internal"]
[null,null,null,32118,20085,"45_Sun Oct 01 2023 16:56:39 GMT+0800","2023-09-29T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Deck fixed Air line found heavily corroded and leaking near No.2 foam monitor.","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","Equipment Related","11.4","Very High","","","Section of the Deck air pipe removed and shifted to workshop. Corroded section of the pipe cropped and renewed. Same Painted & fitted back. ","2023-10-04T23:59:35","","Completed","2023-10-07T23:59:35","No","No","No","Internal"]
[null,null,null,32119,88599,"45_Sun Oct 01 2023 16:52:57 GMT+0800","2023-09-29T23:59:35","Defect","Ship Staff","Ship Staff Insp.","After Re-Inerting operations, During the Inspection of PV Valves prior to load Port, No.5C COT PV Valve found leaking from Pressure side.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.40","High","","","5C PV Valve removed and opened up, Magnets found completely rusted and damaged, Same replaced. Buffing and cleaning of internal components carried out, O-Rings replaced. Lapping and surface cleaning carried out and Tested with onboard testing kit, Found working satisfactory. Same put back in place.","2023-10-02T23:59:35","","Completed","2023-10-02T23:59:35","No","No","No","Internal"]
[null,null,null,32242,13807,"45_Mon Oct 16 2023 11:16:46 GMT+0800","2023-10-07T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Fixed Gas Detection System started giving Flow failure Alarm, Upon investigation it was found that Sampling Pump fan Blade is damaged.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.41","Medium","","","Fan blades were replaced from the old pumps blades which were in good condition. System is working normal - All Satisfactory. Vessel have raised the PO for one Spare Sampling pump as no spares onboard.","2023-10-15T23:59:35","SCAN230265 - VACUUM PUMP FOR GAS DETECTION SYSTEM","Completed","2023-10-15T23:59:35","No","No","No","Internal"]
[null,null,null,32240,56621,"45_Mon Oct 16 2023 19:55:36 GMT+0800","2023-10-12T23:59:35","Non Conformity","Ship Staff","Ship Staff Insp.","Forward Bosun Store Mechanical Fan Mushroom vent is found hard to close due the heavy rusting in the Inner channel guides of the Flap. ","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","Equipment Related","11.6","Medium","","","Complete De-rusting and painting carried after dis-mantling of the Mushroom vent head. Packing and seat inspected, All in order.","2023-11-24T23:59:35","","Completed","2023-10-20T23:59:35","No","No","No","Internal"]
[null,null,null,32421,28343,"45_Mon Nov 06 2023 08:18:05 GMT+0800","2023-10-16T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Port accommodation companion way edge plate corroded & wasted in C-Deck top stair ,  Same to renew","Accommodation","General Appearance","External Factors","11.13","Low","","","Old plate cropped and new plate welded after office Concurrence. Presently all in good order","2024-01-15T23:59:35","","Completed","2023-11-17T23:59:35","No","No","No","Internal"]
[null,null,null,32241,71879,"45_Mon Oct 16 2023 19:59:41 GMT+0800","2023-10-16T23:59:35","Non Conformity","Ship Staff","Ship Staff Insp.","Rubber Packing of the Steering gear room Entrance door on Sunken Deck found to be damaged with multiple cracks. ","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","Equipment Related","11.6","Medium","","","Packing removed. Chipping/Painting of the Channel to be carried out. New Packing put, All in order.","2023-11-27T23:59:35","","Completed","2023-10-21T23:59:35","No","No","No","Internal"]
[null,null,null,32435,86167,"45_Tue Nov 07 2023 09:01:47 GMT+0800","2023-10-17T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Debris found in scrubber ventilation fan mesh .","Elect. Mach. & Equip.","General Appearance","External Factors","10.32","Very High","","","Debris cleared inside the mesh.","2023-11-20T23:59:35","","Completed","2023-10-27T23:59:35","No","No","No","Internal"]
[null,null,null,32436,80896,"45_Tue Nov 07 2023 09:43:37 GMT+0800","2023-10-17T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","3 Weather tight doors in Scrubber tower – have not sighted any full proof means to prevent stowaways entering and hiding inside ","Miscellaneous","ISPS Related","External Factors","7.1","High","","","Locking arrangements from inside fabricated after taking office concurrence.","2024-01-17T23:59:35","","Completed","2023-11-17T23:59:35","No","No","No","Internal"]
[null,null,null,32437,28689,"45_Tue Nov 07 2023 09:49:14 GMT+0800","2023-10-17T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","4 exhaust stacks in funnel renewed in dry dock 2020 not painted.","Miscellaneous","Eng. / Strg. Comp.","External Factors","10.32","Very High","","","4 exhaust stacks in funnel painted with H/R paint .","2023-11-17T23:59:35","","Completed","2023-10-28T23:59:35","No","No","No","Internal"]
[null,null,null,32438,61902,"45_Tue Nov 07 2023 09:53:48 GMT+0800","2023-10-17T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","E/R blower inspection door on funnel deck butterfly nuts jammed .","Miscellaneous","General Appearance","External Factors","10.32","Very High","",""," All 4 blower butterfly nuts greased and freed .","2023-12-27T23:59:35","","Completed","2023-10-27T23:59:35","No","No","No","Internal"]
[null,null,null,32439,70708,"45_Tue Nov 07 2023 09:58:35 GMT+0800","2023-10-17T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","2 pieces of railings  dented on port E/R lower platform","Miscellaneous","Eng. / Strg. Comp.","External Factors","10.32","Very High","","","To repair by cropping and renewing the pipes.","2024-01-17T23:59:35","","Completed","2023-11-13T23:59:35","No","No","No","Internal"]
[null,null,null,32441,59504,"45_Tue Nov 07 2023 08:39:29 GMT+0800","2023-10-17T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Frame of the PA Speaker on the monkey island rusted.","Accommodation","General Appearance","External Factors","11.8","Low","","","Frame  renewed.","2023-11-25T23:59:35","","Completed","2023-10-21T23:59:35","No","No","No","Internal"]
[null,null,null,32442,76723,"45_Tue Nov 07 2023 09:56:18 GMT+0800","2023-10-17T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Scrubber tower louvres on P & S sides very hard to operate.","Miscellaneous","Eng. / Strg. Comp.","External Factors","10.32","Very High","","","freed up and greased. Presently operating freely.","2023-12-17T23:59:35","","Completed","2023-10-25T23:59:35","No","No","No","Internal"]
[null,null,null,32414,45460,"45_Sat Oct 28 2023 08:21:39 GMT+0800","2023-10-21T23:59:35","Observation,Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Emergency cargo valve pump equipment minor leaks to be repaired.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.11","Medium","","","Leakage attended and rectified. Presently pump working properly.","2023-12-30T23:59:35","","Completed","2023-12-01T23:59:35","No","No","No","Internal"]
[null,null,null,32415,30049,"45_Sat Oct 28 2023 08:27:58 GMT+0800","2023-10-21T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Accommodation deck drains found rusted to be chipped and 1/2 metal strips to be welded to prevent drain water getting choked.","Accommodation","ISM Related","Equipment Related","11.13","Low","","","All mesh removed from the Drain, Chipping and Painting  done. Metal strips welded after concurrence from office. Presently all in good order.","2023-11-30T23:59:35","","Completed","2023-11-18T23:59:35","No","No","No","Internal"]
[null,null,null,32417,27159,"45_Fri Nov 03 2023 09:09:53 GMT+0800","2023-10-25T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Fire pump overboard valve (Ship side valve 20V) stuck in close position and very difficult to operate the valve.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","",""," Valve renewed by plugging the overboard valve from outside. Presently all in good order. No leakages observed after trying out. Valve is able to be operated freely.","2024-01-25T23:59:35","SCAN230282","Completed","2023-11-22T23:59:35","No","No","No","Internal"]
[null,null,null,32422,80662,"45_Mon Nov 06 2023 08:24:34 GMT+0800","2023-10-25T23:59:35","Critical Equipment","Ship Staff","Ship Staff Insp.","OWS solenoid recirculation valve on the Marin floc unit not operating when OCM exceeds 15PPM during operation.","Critical Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","trouble shooting done as per maker and office advice. Now working satisfactory.","2024-01-18T23:59:35","","Completed","2023-11-13T23:59:35","No","No","No","Internal"]
[null,null,null,32423,28089,"45_Mon Nov 06 2023 08:36:31 GMT+0800","2023-10-25T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Valve 93V(Butterfly VV) on the fire line overboard damaged and leaking from the sealing. Also the valve actuator gears are corroded and wasted due to the sea water seepage into the actuator.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Valve  renewed with new spare valve. Fire line tried out to 12 bar pressure found no leakage.","2024-01-25T23:59:35","SCAN230282","Completed","2023-12-11T23:59:35","No","No","No","Internal"]
[null,null,null,32418,20548,"45_Fri Nov 03 2023 10:55:19 GMT+0800","2023-10-26T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Standby O2 analyzer unit not giving steady reading. Even after multiple calibration the sensed value is fluctuating.","Inert Gas","","Equipment Related","8.22","Very High","","","Old O2 sensor replaced with spare new one. System calibrated and presently working satisfactorily and showing steady readings.","2024-01-26T23:59:35","PO # SCAN230260","Completed","2023-12-07T23:59:35","No","No","No","Internal"]
[null,null,null,32416,69264,"45_Thu Nov 02 2023 09:42:28 GMT+0800","2023-10-27T23:59:35","Defect","Ship Staff","Ship Staff Insp.","LT cooler#1 leaking from the plates gasket.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Plates to be removed ,gasket inspected and gaskets to be renewed if required. Added in Refman.","2024-01-27T23:59:35","","Completed","2023-11-17T23:59:35","No","No","No","Internal"]
[null,null,null,32428,77235,"45_Mon Nov 06 2023 13:35:40 GMT+0800","2023-10-30T23:59:35","Observation","Ship Staff","Ship Staff Insp.","BA 036 - Discharge Valve for No.1 WBP is full open even in shut condition. After work on VRCS system in DD, same was closing even on neutral position. ","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.18","High","","","Issue found with the switch in CCR panel same renewed. Presently working satisfactorily.","2023-11-30T23:59:35","","Completed","2023-11-29T23:59:35","No","No","No","Internal"]
[null,null,null,32430,66347,"0_Mon Nov 06 2023 13:42:23 GMT+0800","2023-10-30T23:59:35","Observation","Ship Staff","Ship Staff Insp.","OT-105 : 1P COT Main Valve indicator is off by about 30% from the actual position when compared with the Solenoid box located on main deck. So the Valve indication in CCR is 30% open when actually the Valve is shut.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.18","High","","","Trouble-shooting for the same done, Potentiometer replaced with the new spare, Now it is in order.","2023-11-30T23:59:35","","Completed","2023-11-10T23:59:35","No","No","No","Internal"]
[null,null,null,32431,71346,"0_Mon Nov 06 2023 13:49:31 GMT+0800","2023-10-30T23:59:35","Observation","Ship Staff","Ship Staff Insp.","BA 002 : Hydraulically operated Valve for FPK Tank is not showing shut indication. Same was also briefed to HKT Marine technicians during the Dry-dock but the Problem was not resolved.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.18","High","","","Microswitch on the valve position indicator adjusted. Presently showing shut indication in CCR.","2023-12-30T23:59:35","","Completed","2023-12-06T23:59:35","No","No","No","Internal"]
[null,null,null,32429,10354,"0_Mon Nov 06 2023 13:38:46 GMT+0800","2023-10-31T23:59:35","Observation","Ship Staff","Ship Staff Insp.","OT-124 : 4S COT main Valve indicator is showing 20% open even in fully shut condition. Actual shut position of the Valve has been verified from solenoid box on deck.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.18","High","","","Trouble-shooting for the same done. Potentiometer changed by putting the old/used potentiometer, same is working in good condition.","2023-11-30T23:59:35","","Completed","2023-11-10T23:59:35","No","No","No","Internal"]
[null,null,null,32841,53689,"45_Fri Nov 17 2023 13:53:10 GMT+0800","2023-11-02T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Various Stud bolts/nuts of the Dresser coupling on Deck pipelines found to be heavily corroded and wasted at some locations.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","11.4","Very High","","","Rusted & wasted studs and nuts for all All deck pipelines were renewed with the SS Studs and nuts. Greasing and Painting of the same will be done as per Job plan. ","2023-11-20T23:59:35","","Completed","2023-11-15T23:59:35","No","No","No","Internal"]
[null,null,null,32842,82954,"45_Sat Nov 11 2023 14:05:11 GMT+0800","2023-11-06T23:59:35","Critical Equipment","Ship Staff","Ship Staff Insp.","As per the safety circular released by the Marshall Island flag the CO2 system manufactured and installed on vessels prior 2016,having the bursting discs made of copper to be replaced with nickel bursting disc.","Critical Equip.,LSA / FFA","Safety / LSA / FFA","Industry Issue","5.40","Very High","","","Job shifted to Dry Dock.","2024-01-06T23:59:35","","Completed","2023-11-17T23:59:35","No","No","No","Internal"]
[null,null,null,32434,89398,"45_Mon Nov 06 2023 15:49:27 GMT+0800","2023-11-06T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Galley Aircon & Wash-Basin Drain reported chocked by the Galley staff. On Investigation, found that whole drain line of Galley aft bulkhead area is chocked.","Accommodation","MLC Related","Human Error","11.13","Low","","","Vessel requested concurrence from office  for the Hot work to cut the Chocked pipe section in the Provision, Clear the drain and make flange arrangement for future use. Job completed.","2023-11-21T23:59:35","","Completed","2023-11-17T23:59:35","No","No","No","Internal"]
[null,null,null,32844,15393,"0_Fri Nov 17 2023 14:02:48 GMT+0800","2023-11-10T23:59:35","Defect","Ship Staff","Ship Staff Insp.","during the Maintenance of the Provision crane(Stbd), During De-rusting, one of the coupling started leaking. ","Deck - Machinery","Structural Condn. / WT integrity ","Equipment Related","8.50","Medium","","","Leak rectified by welding the coupling connectors in workshop and fitted back in place, tried out the crane found no leaks presently. Vessel shall order Spare connectors.","2023-11-21T23:59:35","","Completed","2023-11-20T23:59:35","No","No","No","Internal"]
[null,null,null,32846,57466,"45_Fri Nov 17 2023 13:59:04 GMT+0800","2023-11-13T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Mooring winch Isolation valve for MW 13/14 winch found leaking. Upon close-up inspection, found that the Valve body is cracked.","Deck - Mooring Machinery","Mooring","Equipment Related","9.14","Medium","","","Isolation valve renewed with spare new valve onboard. (Same was located in steering gear room). System tried out presently no leaks observed.","2023-11-20T23:59:35","","Completed","2023-11-20T23:59:35","No","No","No","Internal"]
[null,null,null,32848,68278,"0_Fri Nov 17 2023 13:48:18 GMT+0800","2023-11-14T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Air Line in the Poop Deck, China passage area which is penetrating through E/Rm  to Poop Deck is found leaking near the Penetration welding. ","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","Equipment Related","11.4","Very High","","","Section cropped and renewed with new pipe section.","2023-11-21T23:59:35","","Completed","2023-11-20T23:59:35","No","No","No","Internal"]
[null,null,null,32847,39618,"45_Fri Nov 17 2023 14:08:49 GMT+0800","2023-11-15T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Port and Stbd Manifold Drip Trays mesh arrangement is not located. Further Drains going to the 4W's COT are filled with rust and other material waste.","Deck - Pipe / Fittings","Cargo / Ballast Systems","External Factors","6.6","Medium","","","Drains cleared and made operational.","2023-12-10T23:59:35","","Completed","2023-11-20T23:59:35","No","No","No","Internal"]
[null,null,null,32843,58358,"45_Fri Nov 17 2023 15:13:33 GMT+0800","2023-11-16T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Safety Rails for No. 6 & No. 7 foam monitor platform are bend.","LSA / FFA","Safety / LSA / FFA","External Factors","","","","","Safety rails bend rectified.","2023-11-30T23:59:35","","Completed","2023-11-27T23:59:35","No","No","No","Internal"]
[null,null,null,32845,72095,"45_Fri Nov 17 2023 13:44:45 GMT+0800","2023-11-16T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Deck fixed Airline corroded and leaking near no.5 COT area.","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","Equipment Related","11.4","Very High","","","Airline section removed from place, wasted section of the pipe renewed. Pipe pit back in place. No leakage observed after trying out.","2023-11-21T23:59:35","","Completed","2023-11-20T23:59:35","No","No","No","Internal"]
[null,null,null,null,21992,"45_Wed Dec 13 2023 14:24:06 GMT+0800","2023-12-10T08:00:00","Defect","Ship Staff","Ship Staff Insp.","FWG#1 ejector pump suction filter casing found badly damaged and corroded and leaking. New spare filter casing kept on store used as replacement but found the new casing leaking due to damage in casing (Found crack on the casing as well as the body). Same needs to be used after repairs.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","External Factors","10.32","Very High","","","Filter casing to be renewed.","2024-03-10T08:00:00","","Completed","2023-12-15T08:00:00","No","No","No","Internal"]
[null,null,null,null,26918,"45_Fri Nov 17 2023 13:38:50 GMT+0800","2023-11-15T08:00:00","Observation","Ship Staff","Ship Staff Insp.","Forward Bosun Store Davit is Heavily rusted and Material Failure is visible at multiple locations.","Deck - Machinery","Structural Condn. / WT integrity ","External Factors","8.50","Medium","","","Chippied buffed primered and final coated. jo completed","2024-01-30T08:00:00","","Completed","2023-12-17T08:00:00","No","No","No","Internal"]
[null,null,null,null,33458,"45_Wed Jan 10 2024 09:09:47 GMT+0800","2024-01-10T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Aux Engine No..3  Emergency stop  fuel quick closing valve found sluggish when tested.  ","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Valve overhauled presently operating properly.","2024-01-31T08:00:00","","Completed","2024-01-15T08:00:00","No","No","No","Internal"]
[null,null,null,null,60007,"45_Wed Dec 13 2023 14:00:52 GMT+0800","2023-12-13T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Soot collecting tank suction line from the tank heavily corroded. Line is directly attached to the tank. Line needs to be replaced after taking hot work concurrence from office.","Miscellaneous","Eng. / Strg. Comp.","External Factors","10.32","Very High","","","Suction  line replaced .","2024-03-13T08:00:00","","Completed","2024-01-17T08:00:00","No","No","No","Internal"]
[null,null,null,null,34323,"45_Tue Jan 09 2024 11:58:43 GMT+0800","2024-01-09T08:00:00","Defect","Ship Staff","Ship Staff Insp.","solenoid valve for fresh supply to Waste disposer in galley is erratic as it sometimes supplies water and sometimes it doesn't","Accommodation","MARPOL Related","Equipment Related","11.13","Low","","","Solenoid valve repaired. Presently working fine.","2024-03-09T08:00:00","SCAN240003","Completed","2024-01-15T08:00:00","No","No","No","Internal"]
[null,null,null,null,39142,"45_Wed Jan 24 2024 22:15:13 GMT+0800","2024-01-19T08:00:00","Defect","Ship Staff","Ship Staff Insp.","No.2 ME F.O. Circulating pump found leaking heavily from shaft seal and making abnormal  noise.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","New mechanical seal and bearing fitted. All seals replaced with new ones. Pump fitted and tested. Found to be satisfactory. All parameters are normal.","2024-02-29T08:00:00","","Completed","2024-01-23T08:00:00","No","No","No","Internal"]
[null,null,null,null,22820,"45_Wed Jan 24 2024 22:47:09 GMT+0800","2024-01-19T08:00:00","Observation","Ship Staff","Ship Staff Insp.","No.2 ME F.O. Supply pump shaft seal leaking and pump not building sufficient pressure.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","New spares received and pump overhauled using repair kit.  Pump tried out. Found satisfactory.","2024-02-29T08:00:00","","Completed","2024-01-25T08:00:00","No","No","No","Internal"]
[null,null,null,null,62900,"45_Tue Jan 30 2024 20:31:01 GMT+0800","2024-01-19T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Deck F.W. Pipes found cracked in many places due to cold burst crack.  ","Deck - Pipe / Fittings","General Appearance","Equipment Related","","","","","Pipes fabricated as per sizes and few pipes only section portion renewed. All pipes painted and fitted in place.","2024-03-15T08:00:00","","Completed","2024-01-31T08:00:00","No","No","No","Internal"]
[null,null,null,null,69568,"45_Wed Jan 24 2024 22:44:41 GMT+0800","2024-01-19T08:00:00","Breakdown","Ship Staff","Ship Staff Insp.","Sewage  system  becomes frequent in-operational due to clogged sewage pipelines. ","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","New pipes received at last Singapore call.  Pipeline being renewed section by section. All clogged and reduced inner diameter  pipes renewed. Presently sewage evac system found to be operational without any issues.","2024-02-29T08:00:00","","Completed","2024-01-29T08:00:00","No","No","No","Internal"]
[null,null,null,null,81775,"45_Tue Jan 09 2024 11:50:14 GMT+0800","2024-01-09T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Sometimes 2C IG Pressure shows communication error on the IG console on bridge and CCR cargo control panel","Inert Gas","Cargo / Ballast Systems","Equipment Related","8.13","Medium","","","IG sensor renewed","2024-03-08T08:00:00","","Completed","2024-01-31T08:00:00","No","No","No","Internal"]
[null,null,null,null,10820,"45_Wed Jan 17 2024 11:46:33 GMT+0800","2024-01-17T08:00:00","Observation","Ship Staff","Ship Staff Insp.","12 Nos stauntions for safe access to bow (stauntions missing near midship area and forward of break of accommodation) not on board","Deck - Pipe / Fittings","Safety / LSA / FFA","Inappropriate Procedure","12.9","High","","","New stauntions  pipes fabricated. ","2024-03-16T08:00:00","PO# SCAN240008","Completed","2024-02-08T08:00:00","No","No","No","Internal"]
[null,null,null,null,13623,"45_Fri Feb 09 2024 15:08:36 GMT+0800","2024-02-04T08:00:00","Defect","Ship Staff","Ship Staff Insp.","W19 stern mooring winch was observed to be leaking during operation of operating lever","Deck - Mooring Machinery","Mooring","Equipment Related","9.14","Medium","","","Operating lever block removed , O-ring renewed and leak rectified and fixed back","2024-03-31T08:00:00","","Completed","2024-02-12T08:00:00","No","No","No","Internal"]
[null,null,null,null,73270,"45_Tue Jan 09 2024 12:00:18 GMT+0800","2024-01-09T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Garbage compactor has minute hydraulic leak during operation","Accommodation","MARPOL Related","Equipment Related","6.20","Medium","","","Leak rectified by tightening the hydraulic coupling ","2024-03-08T08:00:00","","Completed","2024-02-12T08:00:00","No","No","No","Internal"]
[null,null,null,null,30872,"45_Fri Nov 17 2023 14:22:38 GMT+0800","2023-11-17T08:00:00","Defect","Ship Staff","Ship Staff Insp.","E/R Workshop Aircon evaporator frame badly corroded and wasted beyond repairs., although working. ","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","It has been decided that the condition of Evaporator can be managed and presently no new Package AC is not required.  Hence  job is closed.","2024-02-17T08:00:00","","Completed","2024-02-07T08:00:00","No","No","No","Internal"]
[null,null,null,null,43049,"45_Thu Feb 15 2024 10:26:24 GMT+0800","2024-02-05T08:00:00","Observation","Ship Staff","Ship Staff Insp.","ER Workshop floor paint coating found in many layers  which was done in past  and peeling off at various places due to ageing. It  doesn't  give good cosmetic appearance. ","Miscellaneous","General Appearance","Equipment Related","10.29","Medium","","","Complete chipping and removal of peel off carried out..  Upon removal of old paint floor neatly cleaned and new paint coating  carried out. ","2024-02-29T08:00:00","","Completed","2024-02-18T08:00:00","No","No","No","Internal"]
[null,null,null,null,40450,"45_Thu Feb 15 2024 10:11:00 GMT+0800","2024-02-10T08:00:00","Critical Equipment","Ship Staff","Ship Staff Insp.","Incinerator one portion refractory found in bad condition. near sluice door. ","Critical Equip.","MARPOL Related","Equipment Related","","","","","Incinerator furnace refractory peeled off portion repaired. Sluice door de-attached refractory repaired. Job completed.","2024-03-30T08:00:00","","Completed","2024-02-19T08:00:00","No","No","No","Internal"]
[null,null,null,null,81247,"45_Thu Feb 15 2024 10:00:01 GMT+0800","2024-02-07T08:00:00","Defect","Ship Staff","Ship Staff Insp.","No.1 Boiler water Circ Pump  Discharge valve found  not holding. ","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Discharge valve replaced with new one. ","2024-04-15T08:00:00","","Completed","2024-02-27T08:00:00","No","No","No","Internal"]
[null,null,null,null,92633,"45_Fri Feb 09 2024 15:04:49 GMT+0800","2024-02-03T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Port side hose handling crane was observed to be leaking from the Operating lever area of boom up and boom down ","Deck - Machinery","Cargo / Ballast Systems","Equipment Related","8.50","Medium","","","Luffing control lever end cover O-ring replaced. Cover looks slightly deformed. New spare ordered. Presently leak has been rectified. Load test carried out. Found satisfactory.","2024-05-08T08:00:00","","Completed","2024-02-20T08:00:00","No","No","No","Internal"]
[null,null,null,null,97262,"45_Fri Nov 17 2023 14:12:21 GMT+0800","2023-10-17T08:00:00","Critical Equipment","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Stbd Iifeboat wire release stopper plate found wasted.","LSA / FFA","Safety / LSA / FFA","External Factors","5.28","Very High","","","Stopper plate found corroded cropped and new plate fitted in place by drilling. Job completed.","2024-01-31T08:00:00","","Completed","2023-12-20T08:00:00","No","No","No","Internal"]
[null,null,null,null,71817,"45_Mon Nov 06 2023 14:01:05 GMT+0800","2023-10-30T08:00:00","Observation","Ship Staff","Ship Staff Insp.","Mooring Brake testing Kit - Hydraulic Jack started leaking during the testing of Winch brakes for MW20 drum. Leakage is from the Top of the jack during the application of pressure.","Deck - Mooring Machinery","Mooring","Equipment Related","9.7","Medium","","","Ones et of spare O-ring fitted and tested. No leaks noted. Hence job closed.","2024-01-30T08:00:00","PO # SCAN230269","Completed","2024-01-05T08:00:00","No","No","No","Internal"]
[null,null,null,null,43412,"45_Tue Jan 09 2024 11:44:06 GMT+0800","2024-01-09T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Port side windlass hydraulic brake seal leaking when used during operation. ","Deck - Machinery","Mooring","Equipment Related","9.15","Medium","","","Recently  inspected the brake cylinder and found no leaks during operating the hyd brake cylinder. Hence job is closed.","2024-03-08T08:00:00","SCAN230269","Completed","2024-02-20T08:00:00","No","No","No","Internal"]
[null,null,null,null,14353,"45_Fri Nov 11 2022 09:20:05 GMT+0800","2022-10-22T08:00:00","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Main Deck spot derusting and complete deck coating","Miscellaneous","General Appearance","External Factors","11.3","Medium","","","Job has been completed for midship to accommodation by ships crew , spot chipping and painting from fwd to midship was carried out in drydock. and some rust areas near port side forward and forecastle deck completed by ships crew","2024-01-28T08:00:00","","Completed","2024-01-28T08:00:00","No","No","No","Internal"]
[null,null,null,null,97590,"45_Sun Mar 17 2024 12:39:33 GMT+0800","2024-03-11T08:00:00","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Port boiler one of the gauge glass light was not working.","E/R - Boiler,Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","Port Boiler gauge glass bulb renewed","2024-03-16T08:00:00","","Completed","2024-03-12T08:00:00","No","No","No","Internal"]
[null,null,null,null,64512,"45_Sun Mar 17 2024 12:58:41 GMT+0800","2024-03-11T08:00:00","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Boiler feed water pump controller valves leaking from gland. ","E/R - Boiler,E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Gland packing renewed","2024-03-18T08:00:00","","Completed","2024-03-14T08:00:00","No","No","No","Internal"]
[null,null,null,null,75514,"45_Sun Mar 17 2024 16:03:29 GMT+0800","2024-03-11T08:00:00","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Securing chains on main deck to derust and paint","Deck - Pipe / Fittings","Safety / LSA / FFA","External Factors","11.8","Low","","","all chains derusted and painted.","2024-03-26T08:00:00","","Completed","2024-03-16T08:00:00","No","No","No","Internal"]
[null,null,null,null,52154,"45_Sun Mar 17 2024 16:09:20 GMT+0800","2024-03-11T08:00:00","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Both windlass gear case gauge glass painted in green. To clean and check all the winch gear case glass as well.","Deck - Machinery","Mooring","Inappropriate Procedure","9.14","Medium","","","all sight glasses cleaned and cleared of paint","2024-03-21T08:00:00","","Completed","2024-03-16T08:00:00","No","No","No","Internal"]
[null,null,null,null,62337,"45_Sun Mar 17 2024 16:12:41 GMT+0800","2024-03-11T08:00:00","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Stbd side DO bunker flange at manifold to derust and paint , bolts and nuts to renew.","Deck - Pipe / Fittings","General Appearance","External Factors","6.8","High","","","chipped and painted, bolts and nuts found to be in good condition","2024-03-26T08:00:00","","Completed","2024-03-16T08:00:00","No","No","No","Internal"]
[null,null,null,null,11824,"45_Sun Mar 17 2024 16:16:20 GMT+0800","2024-03-11T08:00:00","Other,Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Both bridge wing Gyro stand support flange to renew","Accommodation","Navigation","External Factors","4.9","Medium","","","Vessel received concurrence from office on 18/03/24 and carried out hot work on 19/03/2024 and work completed","2024-04-10T08:00:00","","Completed","2024-03-19T08:00:00","No","No","No","Internal"]
[null,null,null,null,17727,"45_Sun Mar 17 2024 13:01:06 GMT+0800","2024-03-11T08:00:00","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Aft deck hydraulics no 2 hydraulic pump press gauge is not connected to the pump.","Deck - Machinery","Eng. / Strg. Comp.","Equipment Related","","","","","Pressure gauge connection fabricated and connected to the pump. Pump tried out and working satisfactory","2024-03-21T08:00:00","","Completed","2024-03-23T08:00:00","No","No","No","Internal"]
[null,null,null,null,39817,"45_Sun Mar 17 2024 12:54:47 GMT+0800","2024-03-11T08:00:00","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","One plate repaired during docking is not yet painted. Location boiler FD fan platform Stbd side.","Miscellaneous","General Appearance","Inappropriate Procedure","","","","","Cleaning and painting carried out.","2024-03-16T08:00:00","","Completed","2024-03-18T08:00:00","No","No","No","Internal"]
[null,null,null,null,49574,"45_Sun Mar 17 2024 13:04:17 GMT+0800","2024-03-11T08:00:00","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ME FO heater leaking from the steam side. ","E/R - Pipes/ valves & fittings,E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Vessel has renewed the end cover gaskets.","2024-03-26T08:00:00","","Completed","2024-03-25T08:00:00","No","No","No","Internal"]
[null,null,null,null,46454,"45_Sun Feb 25 2024 18:18:49 GMT+0800","2024-02-19T08:00:00","Observation","Ship Staff","Ship Staff Insp.","EGCS Dampers and sealing air lines to be inspected for their proper operation. ","E/R - Pipes/ valves & fittings","MARPOL Related","Equipment Related","10.4","High","","","As per office instruction, EGCS Damper and sealing air lines to be inspected. The condition of by-pass and dampers checked. Job carried out during stoppage of EGCS.","2024-03-31T08:00:00","","Completed","2024-03-25T08:00:00","No","No","No","Internal"]
[null,null,null,null,50644,"45_Wed Dec 13 2023 14:18:43 GMT+0800","2023-12-10T08:00:00","Defect","Ship Staff","Ship Staff Insp.","AE FO supply pump#1 leaking from mechanical seal. Seal needs to be replaced. No spare seal onboard. ","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Presently there is no leak. Vessel will renew the seal if there is any leak observed in the future. Vessel has received the spare under PO No.SCAN240034","2024-03-15T08:00:00","SCAN240034","Completed","2024-03-26T08:00:00","No","No","No","Internal"]
[null,null,null,null,60403,"45_Mon Nov 06 2023 08:49:54 GMT+0800","2023-11-01T08:00:00","Observation","Ship Staff","Ship Staff Insp.","Conduit Pipe in the Starboard Side Life boat going to Stbd Navigation Side-Light is wasted just before the fish Plate area. Same needs to be cropped and renewed.","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","External Factors","11.4","Very High","","","Conduit Pipe cold work repair carried out.","2024-01-15T08:00:00","","Completed","2024-03-01T08:00:00","No","No","No","Internal"]
[null,null,null,null,81142,"45_Sun Oct 01 2023 15:53:37 GMT+0800","2023-09-13T08:00:00","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Steering Gear room door from engine room was found bent and not closing properly. To rectify.","LSA / FFA","","Equipment Related","10.43","Medium","","","Vessel has renewed both doors from engine room to Steering gear. Presently closing positively. ","2024-03-30T08:00:00","SCAN230256","Completed","2024-03-29T08:00:00","No","No","No","Internal"]
[null,null,null,20222,null,"45_31/07/2021 3:36:05 PM","2021-09-22T08:00:00","Observation","Ship Staff","Ship Staff Insp.","AE flow meter not working properly. Fuel oil consumtion and flow meter readings are irrelavent most of the times..","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","New flowmeter  and Display unit received  and  Flow meter made operational.","2024-03-30T08:00:00","SCAN245002","Completed","2024-03-22T08:00:00","No","No","No","Internal","on Order. Will be supplied once ready. Target date revised accordingly."]
[null,null,null,null,94380,"45_Tue Jan 31 2023 15:41:21 GMT+0800","2023-01-19T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Safety rings not installed on all E/R  lube oil storage tank ladders.","Hull & Tanks","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Safety Rings fabricated and installed on ER lube oil tank ladders. ","2024-03-30T08:00:00","","Completed","2024-04-20T08:00:00","No","No","No","Internal"]
[null,null,null,null,95356,"45_Fri Nov 03 2023 10:59:48 GMT+0800","2023-11-01T08:00:00","Observation","Ship Staff","Ship Staff Insp.","No fixed drain pipe provided in all COPT drain pot to the scuppers. Presently all the drain pots in COPT are connected to the scupper by flexible hoses.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Fixed drain pipes fabricated with new pipe lines","2024-03-30T08:00:00","","Completed","2024-05-04T08:00:00","No","No","No","Internal"]
[null,null,null,null,79303,"45_Tue Jan 09 2024 12:08:31 GMT+0800","2024-01-09T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Stbd side grating of hose handling crane Platform need to be renewed as extensively corroded","Deck - Pipe / Fittings","Safety / LSA / FFA","External Factors","8.5","Very High","","","Vessel intends to renew gratings \nGratings have been cut to size, however welding work is required which will be carried out in due course in ER workshop.\n\nWelding has been carried out, need to paint and fix back.\n\nWasted gratings of stbd HHC have been renewed.","2024-03-20T08:00:00","","Completed","2024-05-07T08:00:00","No","No","No","Internal"]
[null,null,null,null,55934,"45_Wed Dec 13 2023 13:48:36 GMT+0800","2023-12-10T08:00:00","Defect,Breakdown","Ship Staff","Ship Staff Insp.","MCSW PP#3 found leaking from seal same opened up for overhauling found the sleeve badly corroded and damaged. Temporary repairs carried out on the sleeve and seal renewed. Pump boxed back and tried out. Found vibration on the pump due to the irregular surface of the sleeve. Sleeve needs to be replaced.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","MCSW#3 overhauling carried out, Sleeve, shaft and mechanical seal renewed. Pump tried out and found all in order.","2024-03-20T08:00:00","SCAN240018","Completed","2024-05-07T08:00:00","No","No","No","Internal"]
[null,null,null,null,34587,"45_Sun Oct 01 2023 16:46:40 GMT+0800","2023-09-10T08:00:00","Observation","Ship Staff","Ship Staff Insp.","Rectifier No.1 was giving High temperature alarm during the operation. Same had to be isolated to carry out the BWE Operation.","Miscellaneous","Cargo / Ballast Systems","Equipment Related","6.21","High","","","After fixing AC unit also while ER temp is above 39 Deg rectifier unable to be operated. No problems faced during cold climate. To monitor again in tropical weather. \n\nIn hot climates, additional cooling fans used to cool rectifier units. Also rectifiers can be alternately used during ballasting operations so that they are sufficiently cooled down.","2024-03-25T08:00:00","","Completed","2024-05-09T08:00:00","No","No","No","Internal"]
[null,null,null,null,96644,"45_Wed May 08 2024 12:25:26 GMT+0800","2024-04-12T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Aux .Engine No.1 pneumatic valve for mechanical overspeed device malfunctioned  and activated the stop cylinder.","E/R - Aux. Engine,E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.30","High","","","Pneumatic valve replaced with new spare and system function tested, found in good working order.","2024-06-10T08:00:00","","Completed","2024-05-10T08:00:00","No","No","No","Internal"]
[null,null,null,null,12223,"45_Wed Apr 17 2024 07:51:52 GMT+0800","2024-04-16T08:00:00","Critical Equipment","Ship Staff","Ship Staff Insp.","Analyse pump or internal leakage aalrm no 3 on pump room gas detection system has been received","Accommodation","Safety / LSA / FFA","Equipment Related","5.22","High","","","Sampling pump was not developing sufficient pressure, same made operational using old spare pump valve plate available onboard and system made operational. Presently working without any issue.","2024-07-15T08:00:00","","Completed","2024-05-09T08:00:00","No","No","No","Internal"]
[null,null,null,null,25232,"45_Mon Nov 06 2023 09:02:18 GMT+0800","2023-11-25T08:00:00","Other,Observation","Ship Staff","Ship Staff Insp.","Conduit Pipe in the Port Side Life boat going to Port Side Life raft Launching & lifeboat Embarkation Light is wasted at two sections. Same needs to be completely renewed.","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","External Factors","11.4","Very High","","","Cold repair has been carried out on the conduit line. Condition is satisfactory.","2024-03-30T08:00:00","","Completed","2024-02-01T08:00:00","No","No","No","Internal"]
[null,null,null,null,14190,"45_Sat May 25 2024 16:54:07 GMT+0800","2024-05-24T08:00:00","Defect","Ship Staff","Ship Staff Insp.","16k/6k steam pressure reducing valve actuator found non operational/ hard to operate manually.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Valve actuator eased up and Diaphragm inspected. Diaphragm found damaged, same renewed and valve open /close tried out manually.",null,"","Completed","2024-05-25T08:00:00","No","No","No","Internal"]
[null,null,null,null,57641,"45_Sun May 26 2024 07:36:15 GMT+0800","2024-05-03T08:00:00","Breakdown","Ship Staff","Ship Staff Insp.","No.1P WBT stripper valve was found to be leaking.","Hull & Tanks","Cargo / Ballast Systems","Equipment Related","8.11","Medium","","","Job carried out with all safety precautions in place. Tank entry was made and seat ring renewed. \nValve tested by ballast eductor, found holding.","2024-06-15T08:00:00","","Completed","2024-05-18T08:00:00","No","No","No","Internal"]
[null,null,null,null,52869,"45_Sun May 26 2024 07:39:11 GMT+0800","2024-05-03T08:00:00","Breakdown","Ship Staff","Ship Staff Insp.","No. 5P WBT main valve was found leaking","Hull & Tanks","Cargo / Ballast Systems","Equipment Related","8.11","Medium","","","Tank entry was carried out with all safety measures in place.\nSeat ring of valve was found to be damaged.\nSame was renewed.\nValve was tried out while running eductor, found operating satisfactorily.","2024-06-15T08:00:00","","Completed","2024-05-21T08:00:00","No","No","No","Internal"]
[null,null,null,null,16700,"45_Sun May 26 2024 21:02:26 GMT+0800","2024-05-04T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Lifeboat water ingress","LSA / FFA","Safety / LSA / FFA","Equipment Related","12.14","High","","","Water ingress located from door packing only after testing. Door packing modified for proper sealing and retested without any leak.","2024-06-30T08:00:00","","Completed","2024-05-24T08:00:00","No","No","No","Internal"]
[null,null,null,null,58558,"45_Sun May 26 2024 20:29:56 GMT+0800","2024-05-08T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Battery isolator on one side lifeboat is 120A same needs to be replaced with 80A isolator same as other side life boat","Elect. Mach. & Equip.","Safety / LSA / FFA","Equipment Related","10.3","Medium","","","New battery isolator received onboard and replaced.","2024-06-30T08:00:00","SCAN240140","Completed","2024-05-31T08:00:00","No","No","No","Internal"]
[null,null,null,null,99744,"45_Sun May 26 2024 20:04:17 GMT+0800","2024-05-15T08:00:00","Observation","Ship Staff","Ship Staff Insp.","Port side lifeboat battery charging plug is not not waterproof, same needs to be renewed.","LSA / FFA","Safety / LSA / FFA","Equipment Related","12.14","High","","","New battery charging plug received and installed.","2024-06-30T08:00:00","SCAN240140","Completed","2024-05-31T08:00:00","No","No","No","Internal"]
[null,null,null,null,98867,"45_Sat May 25 2024 16:22:00 GMT+0800","2024-05-16T08:00:00","Defect","Ship Staff","Ship Staff Insp.","ME unit No.5 PCO non-flow alarm received  and Engine slow down activated, upon investigation found the level sensor faulty. ","E/R - Main Engine,Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","New sensor received tested and installed in place.","2024-06-30T08:00:00","SCAN240138","Completed","2024-05-29T08:00:00","No","No","No","Internal"]
[null,null,null,null,93801,"45_Fri May 31 2024 05:26:19 GMT+0800","2024-05-12T08:00:00","Defect","Ship Staff","Nav Audit / Verification","Echo sounder :Fwd transducer depth value is not displayed","Navigation - Echo Sounder / Speed Log","Navigation","Equipment Related","4.19","Low","","","Checked at shallow depth area and observed correct reading displayed, only issue that both fwd and aft readings not displayed together. As per system design only one reading will be displayed at a time with selector switch. Same to be investigated at Disch port-Vietnam as UKC fwd and aft will be different.\n\nChecked both Transducers ( Fwd & aft ) for Echo sounder at Thanh Hoa , Vietnam during discharging at Various levels. \nAs per troubleshooting & Previous communication , there is no issue with both fwd and aft draft transducers. \n\nSystem is designed to show depth only from one transducer at a time as per the selector switch positions ( FWD & AFT) including in dual display mode. Same checked & confirmed at Discharge port With about 6 M  aft trim ( Drafts  Fwd.- 10.9 / Aft -16.9 M ) \nHowever, the confusion is created as after changing over selector switch , reading changes as per fwd. & aft Drafts in Display unit but both readings still display shows as Fwd.  or AFT only depending which transducer is selected as  primary.\nNote regarding the same has been posted near Echo Sounder Display\n","2024-08-12T08:00:00","","Completed","2024-06-05T08:00:00","No","No","No","Internal"]
[null,null,null,null,98926,"45_Sat May 18 2024 12:27:27 GMT+0800","2024-05-18T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Conductive meter (Salinometer cell) for measuring the boiler feed water chloride content was found faulty. \nSame confirmed by testing the cell in fresh water of chloride content less than 10 PPM and found the reading from the cell to be 50 PPM.\n","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.30","High","","","Conductive cell renewed with newly received cell. Conductive reading confirmed by testing chloride content manually. Found satisfactory.","2024-06-30T08:00:00","SCAN230249","Completed","2024-06-11T08:00:00","No","No","No","Internal"]
[null,null,null,null,34714,"45_Wed May 22 2024 19:57:23 GMT+0800","2024-05-07T08:00:00","Defect","Ship Staff","Ship Staff Insp.","04 Nos of Window wiper blades in use were damaged. Out of 7 spare blades available onboard only one blade was usable, rest all blades were old used and damaged. 01 blade replaced and for  new blades RO raised.","Elect. Mach. & Equip.,Accommodation","Navigation","Equipment Related","","","","","Damaged window wiper blades replaced with new spares received.","2024-06-30T08:00:00","SCAN240135","Completed","2024-06-12T08:00:00","No","No","No","Internal"]
[null,null,null,null,26874,"45_Sun May 26 2024 20:43:05 GMT+0800","2024-05-10T08:00:00","Defect","Ship Staff","Ship Staff Insp.","One torch from helicopter equipment is not working ","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.3","Low","","","New spare received and replaced.","2024-06-30T08:00:00","SCAN240148","Completed","2024-06-10T08:00:00","No","No","No","Internal"]
[null,null,null,null,53107,"45_Sun May 26 2024 20:01:11 GMT+0800","2024-05-15T08:00:00","Defect","Ship Staff","Ship Staff Insp.","9 Pcs foam extinguisher hoses found damaged. ","LSA / FFA","Safety / LSA / FFA","Equipment Related","12.15","High","","","Hoses received at Singapore. Same have been renewed for 9 nos. foam extinguishers.","2024-06-30T08:00:00","SCAN240148","Completed","2024-06-11T08:00:00","No","No","No","Internal"]
[null,null,null,null,99159,"45_Sun May 26 2024 19:57:25 GMT+0800","2024-05-17T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Foam isolation valve No 8  is not holding/leaking.","Deck - Pipe / Fittings","Safety / LSA / FFA","Equipment Related","2.16","Medium","","","Job completed. Valve overhauled and tested. No leak found.\n","2024-06-30T08:00:00","SCAN240156 / Item no. 54","Completed","2024-06-11T08:00:00","No","No","No","Internal"]
[null,null,null,null,41292,"45_Sun May 26 2024 20:20:30 GMT+0800","2024-05-14T08:00:00","Defect","Ship Staff","Ship Staff Insp.","foam monitor leaking (No 1 and No8.) from upper bearing ","Deck - Pipe / Fittings","Safety / LSA / FFA","Equipment Related","12.16","High","","","O-ring for both foam monitor upper bearing renewed. System tested without any leak. ","2024-06-30T08:00:00","","Completed","2024-05-30T08:00:00","No","No","No","Internal"]
[null,null,null,null,23978,"45_Sun May 26 2024 22:57:46 GMT+0800","2024-05-21T08:00:00","Breakdown","Ship Staff","Ship Staff Insp.","1S and 2S WBT sounding pipes are wasted on 1st stringer. ","Hull & Tanks","Cargo / Ballast Systems","Equipment Related","8.12","Medium","","","1 STBD WBT  & 2 STBD WBT sounding pipe cold repair on 1st stringer completed.","2024-06-30T08:00:00","","Completed","2024-05-28T08:00:00","No","No","No","Internal"]
[null,null,null,null,13616,"45_Sun May 26 2024 23:12:33 GMT+0800","2024-05-07T08:00:00","Breakdown","Ship Staff","Ship Staff Insp.","2 Pcs hydro blowers onboard were not operational (Seized)","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.18","High","","","New hydro blowers received onboard at Singapore on 10th June 2024. Same tested for operation and found in good working order.","2024-06-30T08:00:00","SCAN240163","Completed","2024-06-13T08:00:00","No","No","No","Internal"]
[null,null,null,null,66389,"45_Tue Jan 09 2024 16:54:48 GMT+0800","2024-01-09T08:00:00","Defect","Ship Staff","Ship Staff Insp.","NO:1 HFO PURIFIER HEATER SAFETY VALVE FOUND LEAKING","E/R - Purifier","Eng. / Strg. Comp.","Equipment Related","","","","","New safety valve received and replaced.","2024-06-30T08:00:00","PO NO:SCAN240031","Completed","2024-03-11T08:00:00","No","No","No","Internal"]
[null,null,null,null,93110,"45_Sun May 26 2024 21:11:41 GMT+0800","2024-05-01T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Few COW V/v's wheels have thinned down .","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.34","High","","","Spare wheels received at Singapore. 05 nos. COW valve wheels renewed.","2024-06-30T08:00:00","SCAN240156","Completed","2024-06-14T08:00:00","No","No","No","Internal"]
[null,null,null,null,28411,"45_Sun May 26 2024 19:54:45 GMT+0800","2024-05-17T08:00:00","Breakdown,Defect","Ship Staff","Ship Staff Insp.","Foam line Isolating valve No 6 seized.","Deck - Pipe / Fittings","Safety / LSA / FFA","Equipment Related","2.16","Medium","","","Job completed. Valve replaced with the spare isolation valve onboard. Tested and no leak observed.","2024-06-30T08:00:00","","Completed","2024-06-14T08:00:00","No","No","No","Internal"]
[null,null,null,null,47487,"45_Mon Nov 06 2023 13:23:57 GMT+0800","2023-10-16T08:00:00","Observation","Ship Staff","Ship Staff Insp.","One Section of Conduit Pipe atop 4S COT from Centre Conduit box going to 4S Overfill alarm junction box is wasted, same needs to be renewed.","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","External Factors","11.4","Very High","","","Cold repair has been carried out and completed.","2024-06-30T08:00:00","","Completed","2024-06-14T08:00:00","No","No","No","Internal"]
[null,null,null,null,77691,"45_Mon Jun 17 2024 12:14:38 GMT+0800","2024-06-10T08:00:00","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Inspection hole to make in deck hydraulic motor fwd and aft..","Deck - Mooring Machinery","Eng. / Strg. Comp.","Equipment Related","10.30","High","","","Inspection holes drilled near coupling area for easy routine coupling inspection job (6M).","2024-06-25T08:00:00","","Completed","2024-06-13T08:00:00","No","No","No","Internal"]
[null,null,null,null,65223,"45_Mon Jun 17 2024 12:33:06 GMT+0800","2024-06-10T08:00:00","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Bosun store water mist system to try out as no record available.","LSA / FFA","Safety / LSA / FFA","Equipment Related","10.30","High","","","System tried out for Auto activation, all nozzles confirmed cleared without any blockage.","2024-06-25T08:00:00","","Completed","2024-06-14T08:00:00","No","No","No","Internal"]
[null,null,null,null,27217,"45_Sat Jan 13 2024 11:00:45 GMT+0800","2024-01-13T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Air conditioning system#1 dryer filter unit inlet/ outlet valve not holding. Hence unable to change the dryer element. Complete charge of gas needs to emptied/collected in recovery bottles and the valves needs to be replaced. Vessel does not have spare valves. Valves needs to be ordered.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Isolated and dryer elements renewed without any issue.","2024-06-30T08:00:00"," SCAN240100 ","Completed","2024-06-18T08:00:00","No","No","No","Internal"]
[null,null,null,null,27953,"45_Wed May 29 2024 15:40:14 GMT+0800","2024-05-29T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Stbd side navigation light fitting broken.","","Navigation","Equipment Related","10.30","High","","","New fitting received and installed.","2024-06-30T08:00:00","SCAN240173","Completed","2024-06-20T08:00:00","No","No","No","Internal"]
[null,null,null,null,78918,"45_Mon Jun 17 2024 12:30:10 GMT+0800","2024-06-10T08:00:00","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Port windlass hydraulic brake externals to de-rust and paint","Deck - Pipe / Fittings","General Appearance","External Factors","11.5","Medium","","","De-rusting and painting completed.","2024-06-30T08:00:00","","Completed","2024-06-19T08:00:00","No","No","No","Internal"]
[null,null,null,null,13664,"45_Sun May 26 2024 22:07:38 GMT+0800","2024-05-09T08:00:00","Defect","Ship Staff","Ship Staff Insp.","PV Breaker Level gouge Glass will have to be cleaned thoroughly or may be require to be replaced.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.28","Medium","","","PV breaker gauge cleaned. Water/glycol mixture topped up.","2024-07-16T08:00:00","","Completed","2024-06-01T08:00:00","No","No","No","Internal"]
[null,null,null,null,34370,"45_Sun May 26 2024 20:57:30 GMT+0800","2024-05-02T08:00:00","Defect","Ship Staff","Ship Staff Insp.","4P and slop S COT cow valves (gate valve) stuck in close position with spindle broken.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.34","High","","","4P-1 COW valve & Slop S COW valve renewed.","2024-07-20T08:00:00","SCAN240116","Completed","2024-06-17T08:00:00","No","No","No","Internal"]
[null,null,null,null,24581,"45_Mon Jun 17 2024 12:19:50 GMT+0800","2024-06-10T08:00:00","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","One of the sprinkler head on top of aft deck hydraulic tank leaking. Normally there should not be any water in line in stop condition. Troubleshoot and rectify.","LSA / FFA","Emgcy. Systems","Equipment Related","10.3","Medium","","","Solenoid valve to the sprinkler opened and cleaned, no water leaking now.","2024-07-30T08:00:00","","Completed","2024-06-21T08:00:00","No","No","No","Internal"]
[null,null,null,null,25946,"45_Tue Jan 23 2024 10:11:57 GMT+0800","2024-01-20T08:00:00","Defect","Ship Staff","Ship Staff Insp.","During securing of Stbd anchor after picking up Stbd anchor departure singapore it was noticed that brake for the Stbd side anchor is not holding","Deck - Machinery","Mooring","Equipment Related","9.2","Very High","","","Brake has been mechanically tightened and observed to be holding.","2024-07-30T08:00:00","","Completed","2024-06-23T08:00:00","No","No","No","Internal"]
[null,null,null,null,21655,"45_Sun May 26 2024 22:02:55 GMT+0800","2024-05-10T08:00:00","Defect","Ship Staff","Ship Staff Insp.","WBT tank dome hatch covers are hard to open and few of them require chain block to open .","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.18","High","","","1P, 1S, 3P WBT domes overhauled. WBT domes in good condition.","2024-07-31T08:00:00","","Completed","2024-06-20T08:00:00","No","No","No","Internal"]
[null,null,null,null,62347,"45_Sun May 26 2024 20:53:31 GMT+0800","2024-05-14T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Slop Stbd and 4 Port COT IG isolation valves not holding , seat rings needs to be renewed","Inert Gas","Cargo / Ballast Systems","Equipment Related","","","","","Slop S IG isolation valve replaced with old used spare onboard, found satisfactory. 4P IG isolation valve to b planned.","2024-07-31T08:00:00","SCAN240169","Completed",null,"No","No","No","Internal"]
[null,null,null,null,85894,"45_Mon Oct 16 2023 11:17:52 GMT+0800","2023-10-10T08:00:00","Defect","Ship Staff","Ship Staff Insp.","ME Jacket water temperature controller faulty/Hunting.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","AMS reconfigured by Kongsberg technician on 10th June 2024. AMS to DPU signal was correct but the controller was hunting. Zero and span adjustment done for IP controller as per manual. Controller has been put in to use and presently working in AUTO.","2024-07-31T08:00:00","","Completed","2024-06-26T08:00:00","No","No","No","Internal"]
[null,null,null,null,82796,"45_Tue Jan 09 2024 12:04:28 GMT+0800","2024-01-09T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Aft stern winches  W17,18,19,20 - Have their brake band bottom metal frame thin down due to age and soot deposits","Deck - Machinery","Mooring","Equipment Related","9.15","Medium","","","Winches W17, W18, W19, W20 brake bands renewed.","2024-07-31T08:00:00","SCAN240156","Completed","2024-06-17T08:00:00","No","No","No","Internal"]
[null,null,null,null,94296,"45_Mon Jun 17 2024 12:22:22 GMT+0800","2024-06-10T08:00:00","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ME LO auto backwash filter valve leaking from the shaft seal. To rectify","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.3","Medium","","","Leak rectified.","2024-07-30T08:00:00","","Completed","2024-06-28T08:00:00","No","No","No","Internal"]
[null,null,null,null,71367,"45_Sun May 26 2024 21:38:27 GMT+0800","2024-04-21T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Pump room Lines : Minor Leakage has been observed through flange of V/v no. OP276 ","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.11","Medium","","","Tested during Discharging at Thanh Hoa after tightening the bolts &  no leakage was observed. One more time tested on 04th July while testing No.2 COP & topping off IG in cargo tanks and found no leakage.","2024-07-31T08:00:00","","Completed","2024-07-04T08:00:00","No","No","No","Internal"]
[null,null,null,null,63567,"45_Sat May 25 2024 16:31:52 GMT+0800","2024-05-25T08:00:00","Defect","Ship Staff","Ship Staff Insp.","During last discharging minor leaks reported from No1 and No2 COP, No2 COP bottom seal has been recently renewed.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","During last discharging no leak noticed from No 1 COP, Minor leak noticed from No 2 COP bottom seal. No 2 COP bottom seal has been recently renewed. No 2 bottom seal, stationary seal cover o- ring renewed with original spare. COP tried out with no leakage.","2024-07-31T08:00:00","SCAN240113","Completed","2024-07-04T08:00:00","No","No","No","Internal"]
[null,null,null,null,22353,"45_Sat May 25 2024 16:26:12 GMT+0800","2024-05-08T08:00:00","Defect","Ship Staff","Ship Staff Insp.","IG system not working in AUTO after renewal of PLC","Inert Gas","Cargo / Ballast Systems","Equipment Related","","","","","Service technician attended at Singapore on 10 June 2024.System operation checked, all found working in AUTO.","2024-07-31T08:00:00","","Completed","2024-07-04T08:00:00","No","No","No","Internal"]
[null,null,null,null,29966,"45_Tue Nov 07 2023 15:02:07 GMT+0800","2023-10-12T08:00:00","Observation","Ship Staff","Ship Staff Insp.","No. 3 Cargo Line Stbd side Manifold Remote pressure transmitter is not working. On Trouble-shooting it was found to be faulty.","","Cargo / Ballast Systems","Equipment Related","8.60","High","","","New pressure transmitter received and replaced for No.1 & 3 stbd manifold. Manifold pressure testing carried out using cargo. CCR & local readings comparison carried out, found satisfactory.","2024-07-30T08:00:00","SCAN230299","Completed","2024-07-04T08:00:00","No","No","No","Internal"]
[null,null,null,null,82174,"45_Mon Nov 06 2023 07:59:08 GMT+0800","2023-10-31T08:00:00","Observation","Ship Staff","Ship Staff Insp.","One stud is missing between the cable length of 4 and 5 shackles. Same noted during the Anchoring operations on 31st Oct 2023 in Yeosu, Korea.","Deck - Mooring Machinery","Mooring","Equipment Related","9.20","Medium","","","Job transferred to REFMAN.","2024-07-31T08:00:00","","Completed","2024-07-04T08:00:00","No","No","No","Internal"]

{"sheet":"Calc","index":2,"n_rows":28,"n_cols":12,"rows_kept":28,"cut":false,"hidden":true,"merged":[]}
["Def_type","Def_cause","Equipments","VIQrefno","Observer_code"]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,"Dim itemSele As Long"]
[null,null,null,null,null,null,null,null,null,null,null,"   dim startRow as integer"]
[null,null,null,null,null,null,null,null,null,null,null,"   startRow=1"]
[null,null,null,null,null,null,null,null,null,null,null,"        For itemSele = 0 To ListBox1.ListCount - 1"]
[null,null,null,null,null,null,null,null,null,null,null,"        If ListBox1.Selected(itemSele) = True Then"]
[null,null,null,null,null,null,null,null,null,null,null,"        Worksheets(\"WorksheetName\").Range(\"A\" & startRow).Value = ListBox1.List(itemSele)"]
[null,null,null,null,null,null,null,null,null,null,null,"        startRow = startRow + 1"]
[null,null,null,null,null,null,null,null,null,null,null,"        End If"]
[null,null,null,null,null,null,null,null,null,null,null,"        Next"]
[null,null,null,null,null,null,null,null,null,null,null,"Dim LastRowA As String"]
[null,null,null,null,null,null,null,null,null,null,null,"        Dim itemSele As Long"]
[null,null,null,null,null,null,null,null,null,null,null,"       Dim startRow as integer"]
[null,null,null,null,null,null,null,null,null,null,null,"        LastRowA = ActiveSheet.Cells(Rows.count, \"A\").End(xlUp).row"]
[null,null,null,null,null,null,null,null,null,null,null,"        startQue = 0"]
[null,null,null,null,null,null,null,null,null,null,null,"        For itemSele = 0 To ListBox1.ListCount - 1"]
[null,null,null,null,null,null,null,null,null,null,null,"        For startRow = 1 To LastRowA"]
[null,null,null,null,null,null,null,null,null,null,null,"        If Worksheets(\"WorksheetName\").Range(\"A\" & startRow).Value = ListBox1.List(itemSele) Then"]
[null,null,null,null,null,null,null,null,null,null,null,"        ListBox1.Selected(itemSele) = True"]
[null,null,null,null,null,null,null,null,null,null,null,"        Exit For"]
[null,null,null,null,null,null,null,null,null,null,null,"        End If"]
[null,null,null,null,null,null,null,null,null,null,null,"        Next j"]
[null,null,null,null,null,null,null,null,null,null,null,"        Next"]
[null,null,null,null,null,null,null,null,null,null,null,"        End If"]

{"sheet":"Areaofobs","index":3,"n_rows":17,"n_cols":2,"rows_kept":17,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Cargo / Ballast Systems",11]
["Cert. & Docu.",2]
["Communication",6]
["Crew Management",3]
["Emgcy. Systems",13]
["Eng. / Strg. Comp.",14]
["General Appearance",15]
["Ice Opns.",17]
["ISM Related",7]
["ISPS Related",10]
["MARPOL Related",9]
["MLC Related",4]
["Mooring",12]
["Navigation",5]
["Safety / LSA / FFA",8]
["Structural Condn. / WT integrity ",16]

{"sheet":"Vessel_type","index":4,"n_rows":1,"n_cols":2,"rows_kept":1,"cut":false,"hidden":true,"merged":[]}
["Vessel_type","ID"]

{"sheet":"Deficiency_type","index":5,"n_rows":8,"n_cols":3,"rows_kept":8,"cut":false,"hidden":true,"merged":[]}
["TITLE","Type of deficiency_description","ID"]
["Breakdown",null,6]
["Critical Equipment",null,4]
["Defect",null,1]
["Guarantee Claim",null,8]
["Non Conformity",null,2]
["Observation",null,3]
["Other",null,7]

{"sheet":"VIQrefno","index":6,"n_rows":427,"n_cols":3,"rows_kept":427,"cut":false,"hidden":true,"merged":[]}
["VIQ_ref_no","Risk Value of observation","ID"]
["1.1","Low",8243]
["1.10","Low",8252]
["1.11","Low",8253]
["1.12","Low",8254]
["1.13","Low",8255]
["1.14","Low",8256]
["1.15","Low",8257]
["1.16","Low",8259]
["1.17","Low",8260]
["1.18","Low",8261]
["1.19","Low",8262]
["1.2","Low",8244]
["1.20","Low",8263]
["1.21","Low",8265]
["1.22","Low",8266]
["1.23","Low",8267]
["1.24","Low",8268]
["1.25","Low",8269]
["1.26","Low",8270]
["1.3","Low",8245]
["1.4","Low",8246]
["1.5","Low",8247]
["1.6","Low",8248]
["1.7","Low",8249]
["1.8","Low",8250]
["1.9","Low",8251]
["1.99","High",11258]
["10.1","Medium",8461]
["10.10","High",8470]
["10.11","Medium",8471]
["10.12","Very High",8472]
["10.13","Very High",8473]
["10.14","Medium",8474]
["10.15","Low",8475]
["10.16","Very High",8476]
["10.17","Very High",8477]
["10.18","High",8478]
["10.19","Very High",8479]
["10.2","Low",8462]
["10.20","High",8480]
["10.21","Medium",8481]
["10.22","Low",8482]
["10.23","Medium",8483]
["10.24","Low",8484]
["10.25","Very High",8485]
["10.26","High",8486]
["10.27","Medium",8487]
["10.28","Low",8488]
["10.29","Medium",8489]
["10.3","Medium",8463]
["10.30","High",8490]
["10.31","Very High",8491]
["10.32","Very High",8492]
["10.33","High",8493]
["10.34","High",8494]
["10.35","Very High",8495]
["10.36","Very High",8496]
["10.37","Medium",8497]
["10.38","Medium",8498]
["10.39","High",8499]
["10.4","High",8464]
["10.40","Medium",8500]
["10.41","Medium",8501]
["10.42","Medium",8502]
["10.43","Medium",8503]
["10.44","Medium",8504]
["10.45","Very High",8505]
["10.46","High",8506]
["10.47","Medium",8507]
["10.48","High",8508]
["10.49","Medium",8509]
["10.5","Low",8465]
["10.50","High",8510]
["10.51","Low",8511]
["10.52","Medium",8512]
["10.53","Medium",8513]
["10.54","High",8514]
["10.55","Low",8515]
["10.6","Very High",8466]
["10.7","Medium",8467]
["10.8","Medium",8468]
["10.9","Medium",8469]
["10.99","High",8516]
["11.1","High",8420]
["11.10","Medium",8429]
["11.11","Very High",8430]
["11.12","Low",8431]
["11.13","Low",8432]
["11.14","Medium",8433]
["11.15","Low",8434]
["11.16","Low",8435]
["11.17","Low",8436]
["11.2","Medium",8421]
["11.3","Medium",8422]
["11.4","Very High",8423]
["11.5","Medium",8424]
["11.6","Medium",8425]
["11.7","High",8426]
["11.8","Low",8427]
["11.9","Low",8428]
["11.99","High",8437]
["12.1","High",8438]
["12.10","High",8448]
["12.11","High",8449]
["12.12","High",8450]
["12.13","High",8451]
["12.14","High",8452]
["12.15","High",8453]
["12.16","High",8454]
["12.17","High",8455]
["12.18","High",8456]
["12.19","High",8457]
["12.2","High",8439]
["12.20","High",8458]
["12.21","High",8459]
["12.3","High",8441]
["12.4","High",8442]
["12.5","High",8443]
["12.6","High",8444]
["12.7","High",8445]
["12.8","High",8446]
["12.9","High",8447]
["12.99","High",8460]
["2.1","Very High",8296]
["2.1.9","Very High",11259]
["2.10","Medium",8304]
["2.11","Medium",8305]
["2.12","Low",8306]
["2.13","Low",8307]
["2.14","Low",8308]
["2.15","Low",8309]
["2.16","Medium",8310]
["2.2","Medium",8297]
["2.3","High",8295]
["2.4","Medium",8298]
["2.5","Medium",8299]
["2.6","Low",8300]
["2.7","High",8301]
["2.8","High",8302]
["2.9","Medium",8303]
["2.99","High",8311]
["3.1","High",8312]
["3.2","Very High",8313]
["3.3","High",8314]
["3.4","Low",8294]
["3.5","Medium",8315]
["3.6","High",8316]
["3.7","Very High",8317]
["3.8","Very High",8318]
["3.99","High",8319]
["4.1","High",8320]
["4.10","High",8329]
["4.11","Medium",8330]
["4.12","Very High",8331]
["4.13","Very High",8332]
["4.14","Very High",8333]
["4.15","Very High",8334]
["4.16","Very High",8335]
["4.17","Very High",8336]
["4.18","Very High",8337]
["4.19","Low",8338]
["4.2","Medium",8321]
["4.20","Very High",8339]
["4.21","High",8340]
["4.22","Low",8341]
["4.23","High",8342]
["4.24","High",8343]
["4.25","Low",8344]
["4.26","Low",8345]
["4.27","High",8346]
["4.3","Medium",8322]
["4.4","High",8323]
["4.5","Very High",8324]
["4.6","Medium",8325]
["4.7","High",8326]
["4.8","Medium",8327]
["4.9","Medium",8328]
["4.99","High",8347]
["5.1","Very High",8517]
["5.10","High",8526]
["5.11","Low",8527]
["5.12","Medium",8528]
["5.13","High",8529]
["5.14","Very High",8530]
["5.15","Medium",8531]
["5.16","Very High",8532]
["5.17","Very High",8533]
["5.18","High",8534]
["5.19","Medium",8535]
["5.2","Very High",8518]
["5.20","Medium",8536]
["5.21","Medium",8537]
["5.22","High",8539]
["5.23","Very High",8540]
["5.24","Very High",8541]
["5.25","Medium",8542]
["5.26","Medium",8543]
["5.27","Medium",8544]
["5.28","Very High",8545]
["5.29","High",8546]
["5.3","Low",8519]
["5.30","High",8547]
["5.31","High",8548]
["5.32","High",8549]
["5.33","High",8550]
["5.34","Low",8551]
["5.35","Medium",8552]
["5.36","Low",8553]
["5.37","Low",8554]
["5.38","High",8555]
["5.39","Very High",8556]
["5.4","High",8520]
["5.40","Very High",8557]
["5.41","Very High",8558]
["5.42","Medium",8559]
["5.43","High",8560]
["5.44","High",8561]
["5.45","Medium",8564]
["5.46","Medium",8565]
["5.47","Medium",8566]
["5.48","Medium",8567]
["5.5","Low",8521]
["5.6","Low",8522]
["5.7","Medium",8523]
["5.8","Medium",8524]
["5.9","Very High",8525]
["5.99","High",8568]
["6.1","Medium",8348]
["6.10","Low",8357]
["6.11","High",8358]
["6.12","Medium",8359]
["6.13","Low",8360]
["6.14","High",8361]
["6.15","High",8362]
["6.16","Very High",8363]
["6.17","Very High",8364]
["6.18","Medium",8365]
["6.19","Low",8366]
["6.2","High",8349]
["6.20","Medium",8367]
["6.21","High",8368]
["6.22","Medium",8369]
["6.3","Low",8350]
["6.4","High",8351]
["6.5","Medium",8352]
["6.6","Medium",8353]
["6.7","High",8354]
["6.8","High",8355]
["6.9","Low",8356]
["6.99","High",8370]
["7.1","High",8371]
["7.10","High",8380]
["7.11","High",8381]
["7.12","High",8382]
["7.13","Medium",8383]
["7.14","Medium",8384]
["7.15","High",8385]
["7.16","High",8386]
["7.17","High",8387]
["7.2","High",8372]
["7.3","Low",8373]
["7.4","Low",8374]
["7.5","Low",8375]
["7.6","Medium",8376]
["7.7","Low",8377]
["7.8","High",8378]
["7.9","High",8379]
["7.99","High",8388]
["8.1","Very High",8569]
["8.10","Very High",8578]
["8.100","Low",11227]
["8.101","Medium",11228]
["8.102","Low",11229]
["8.103","Low",11230]
["8.104","Low",11231]
["8.105","Medium",11232]
["8.106","Medium",11233]
["8.107","Low",11234]
["8.108","High",11235]
["8.109","Very High",11236]
["8.11","Medium",8579]
["8.110","High",11237]
["8.111","Medium",11238]
["8.112","High",11239]
["8.113","Medium",11240]
["8.114","Low",11241]
["8.115","High",11242]
["8.116","Medium",11243]
["8.117","Medium",11244]
["8.118","Medium",11245]
["8.119","High",11246]
["8.12","Medium",8580]
["8.120","High",11247]
["8.121","Medium",11248]
["8.122","High",11249]
["8.123","High",11250]
["8.124","Low",11251]
["8.125","High",11252]
["8.126","Medium",11253]
["8.127","Medium",11254]
["8.13","Medium",8581]
["8.14","Very High",8582]
["8.15","High",8583]
["8.16","Very High",8584]
["8.17","Low",8585]
["8.18","High",8586]
["8.19","High",8587]
["8.199","High",11255]
["8.2","Medium",8570]
["8.20","Medium",8588]
["8.21","High",8589]
["8.22","Very High",8590]
["8.23","Medium",8591]
["8.24","Medium",8592]
["8.25","Very High",8593]
["8.26","High",8594]
["8.27","Medium",8595]
["8.28","Medium",8596]
["8.29","High",8598]
["8.3","Very High",8571]
["8.30","High",8599]
["8.31","High",8600]
["8.32","Low",8601]
["8.33","Medium",8602]
["8.34","High",8603]
["8.35","Medium",8604]
["8.36","Medium",8605]
["8.37","High",8607]
["8.38","Medium",8608]
["8.39","Medium",8609]
["8.4","Medium",8572]
["8.40","High",8610]
["8.41","Medium",8611]
["8.42","Medium",8612]
["8.43","Very High",8613]
["8.44","High",8615]
["8.45","High",8616]
["8.46","Very High",8617]
["8.47","Very High",8618]
["8.48","Medium",8619]
["8.49","High",8620]
["8.5","Very High",8573]
["8.50","Medium",8621]
["8.51","Low",8622]
["8.52","Low",8623]
["8.53","Low",8624]
["8.54","High",8625]
["8.55","Low",11182]
["8.56","Medium",11183]
["8.57","Medium",11184]
["8.58","High",11185]
["8.59","High",11186]
["8.6","Medium",8574]
["8.60","High",11187]
["8.61","Medium",11188]
["8.62","Very High",11189]
["8.63","High",11190]
["8.64","Medium",11191]
["8.65","Low",11192]
["8.66","High",11193]
["8.67","High",11194]
["8.68","High",11195]
["8.69","Medium",11196]
["8.7","High",8575]
["8.70","Medium",11197]
["8.71","Very High",11198]
["8.72","Medium",11199]
["8.73","Medium",11200]
["8.74","High",11201]
["8.75","Medium",11202]
["8.76","Medium",11203]
["8.77","Medium",11204]
["8.78","Medium",11205]
["8.79","Medium",11206]
["8.8","Medium",8576]
["8.80","Medium",11207]
["8.81","Low",11208]
["8.82","Medium",11209]
["8.83","Low",11210]
["8.84","Low",11211]
["8.85","Medium",11212]
["8.86","Medium",11213]
["8.87","Medium",11214]
["8.88","Low",11215]
["8.89","High",11216]
["8.9","High",8577]
["8.90","High",11217]
["8.91","High",11218]
["8.92","Medium",11219]
["8.93","Low",11220]
["8.94","Low",11221]
["8.95","Medium",11222]
["8.96","Medium",11223]
["8.97","Low",11224]
["8.98","High",11225]
["8.99","Medium",11226]
["9.1","Low",8390]
["9.10","Medium",8399]
["9.11","Medium",8400]
["9.12","Medium",8401]
["9.13","Low",8402]
["9.14","Medium",8403]
["9.15","Medium",8404]
["9.16","High",8405]
["9.17","High",8406]
["9.18","Low",8407]
["9.19","Low",8408]
["9.2","Very High",8391]
["9.20","Medium",8409]
["9.21","Medium",8410]
["9.22","Low",8411]
["9.23","Low",8412]
["9.24","Medium",8413]
["9.25","Low",8414]
["9.26","Low",8415]
["9.27","Low",8416]
["9.28","Medium",8417]
["9.29","Low",8418]
["9.3","Very High",8392]
["9.4","High",8393]
["9.5","High",8394]
["9.6","Low",8395]
["9.7","Medium",8396]
["9.8","Medium",8397]
["9.9","Medium",8398]
["9.99","High",8419]

{"sheet":"Equipment_list","index":7,"n_rows":28,"n_cols":3,"rows_kept":28,"cut":false,"hidden":true,"merged":[]}
["TITLE","Equipment_list_description","ID"]
["Accommodation",null,12]
["Cargo Mach.",null,13]
["Critical Equip.",null,16]
["Deck - Machinery",null,18]
["Deck - Mooring Machinery",null,15]
["Deck - Pipe / Fittings",null,20]
["Documentation",null,21]
["E/R - Air Comp.",null,8]
["E/R - Aux. Engine",null,4]
["E/R - Aux. Mach.",null,7]
["E/R - Boiler",null,5]
["E/R - Main Engine",null,3]
["E/R - Pipes/ valves & fittings",null,9]
["E/R - Pumps",null,32]
["E/R - Purifier",null,6]
["Elect. Mach. & Equip.",null,10]
["Hull & Tanks",null,19]
["Inert Gas",null,14]
["LSA / FFA",null,17]
["Miscellaneous",null,22]
["Navigation - DGPS / EPFS / AIS",null,28]
["Navigation - ECDIS",null,25]
["Navigation - Echo Sounder / Speed Log",null,26]
["Navigation - GMDSS & Communication",null,23]
["Navigation - Others",null,11]
["Navigation - RADAR",null,24]
["Navigation - VDR / BNWAS",null,30]

{"sheet":"PSC_MOU","index":8,"n_rows":11,"n_cols":3,"rows_kept":11,"cut":false,"hidden":true,"merged":[]}
["TITLE","PSC_MOU_description","ID"]
["Asia and the Pacific",null,2]
["Caribbean",null,4]
["Europe and the North Atlantic",null,1]
["Latin America",null,3]
["The Black Sea region",null,6]
["The Indian Ocean",null,8]
["The Mediterranean",null,7]
["The Riyadh MoU",null,9]
["USCG",null,10]
["West and Central Africa",null,5]

{"sheet":"Inspection_type","index":9,"n_rows":13,"n_cols":2,"rows_kept":13,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Bunkering Audit",14]
["Cargo Audit",17]
["Engineering Audit",16]
["ISM Audit",2]
["ISPS Audit",3]
["IT Audit",10]
["MLC Audit",1]
["Mooring Audit",9]
["Nav Audit / Verification",8]
["Onboard Training",18]
["Ship Staff Insp.",15]
["Suptd. Insp.",13]

{"sheet":"Deficiency_Cause","index":10,"n_rows":8,"n_cols":3,"rows_kept":8,"cut":false,"hidden":true,"merged":[]}
["TITLE","Deficiency_Cause_description","ID"]
["Behaviour Based",null,1]
["Equipment Related",null,4]
["External Factors",null,5]
["Human Error",null,7]
["Inappropriate Procedure",null,8]
["Industry Issue",null,6]
["Knowledge Based",null,3]

{"sheet":"Observer_code","index":11,"n_rows":3,"n_cols":3,"rows_kept":3,"cut":false,"hidden":true,"merged":[]}
["TITLE","Observer_code_description","ID"]
["Owner / Marine / Tech. Suptd.",null,3]
["Ship Staff",null,2]

{"sheet":"Status_code","index":12,"n_rows":6,"n_cols":3,"rows_kept":6,"cut":false,"hidden":true,"merged":[]}
["TITLE","Status_code_description","ID"]
["Completed",null,6]
["Deferred to D D",null,5]
["In progress",null,3]
["Not Started",null,2]
["Waiting spare",null,4]

{"sheet":"PSC_ref_no","index":13,"n_rows":19,"n_cols":2,"rows_kept":19,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Alarms",9]
["Cargo operations including equipment",7]
["Certificates & Documentation",2]
["Dangerous Goods",13]
["Emergency Systems",5]
["Fire safety",8]
["ISM",16]
["ISPS",17]
["Life saving appliances",12]
["MLC, 2006",18]
["Other",19]
["Pollution Prevention",15]
["Propulsion and auxiliary machinery",14]
["Radio communication",6]
["Safety of Navigation",11]
["Structural condition",3]
["Water/Weathertight condition",4]
["Working and Living Conditions",10]

{"sheet":"Risk_value_of_obs","index":14,"n_rows":1,"n_cols":2,"rows_kept":1,"cut":false,"hidden":true,"merged":[]}
["Risk Value of observation","ID"]

{"sheet":"Year","index":15,"n_rows":18,"n_cols":1,"rows_kept":18,"cut":false,"hidden":true,"merged":[]}
["Year"]
[2014]
[2015]
[2016]
[2017]
[2018]
[2019]
[2020]
[2021]
[2022]
[2023]
[2024]
[2025]
[2026]
[2027]
[2028]
[2029]
[2030]

{"sheet":"Month","index":16,"n_rows":13,"n_cols":1,"rows_kept":13,"cut":false,"hidden":true,"merged":[]}
["Month"]
["Jan"]
["Feb"]
["Mar"]
["Apr"]
["May"]
["Jun"]
["Jul"]
["Aug"]
["Sep"]
["Oct"]
["Nov"]
["Dec"]

{"sheet":"Date_","index":17,"n_rows":32,"n_cols":1,"rows_kept":32,"cut":false,"hidden":true,"merged":[]}
["Date"]
["01"]
["02"]
["03"]
["04"]
["05"]
["06"]
["07"]
["08"]
["09"]
[10]
[11]
[12]
[13]
[14]
[15]
[16]
[17]
[18]
[19]
[20]
[21]
[22]
[23]
[24]
[25]
[26]
[27]
[28]
[29]
[30]
[31]

{"sheet":"Sheet1","index":18,"n_rows":24,"n_cols":6,"rows_kept":24,"cut":false,"hidden":true,"merged":[]}
[]
[null,"ID","E",null,"Date Recorded",1]
[null,"UNIQUE ID","F",null,"Type of Deficiency",2]
[1,"Date Recorded","G",null,"Observer code",3]
["ignore","Vessel Type","H",null,"Type of Inspection",4]
[null,"Internal / External","I",null,"Description of Deficiency",5]
[null,"Drydock","J",null,"Equipment Categories",6]
[null,"Information Sharing","K",null,"Area of Observation",7]
[null,"Critical_item","L",null,"Deficiency Cause",8]
[null,"Deficiency Type","M",null,"VIQ Ref Number",9]
[null,"Deficiency Cause","N",null,"Risk Value of Obs",10]
[null,"Inspection Type","O",null,"PSC Ref Number",11]
[null,"Equipments","P",null,"PSC MOU ID",12]
[null,"VIQ Reference Number","Q",null,"Action Taken or Required",13]
[null,"Risk Value of the observation","R",null,"Target Date",14]
[null,"PSC Reference Number","S",null,"PO Ref No.",15]
[null,"PSC MOU","T",null,"Status Code",16]
[null,"Observer Code","U",null,"Date Completed",17]
[null,"Target Date","V",null,"Drydock",18]
[null,"Status Code","W",null,"Info Sharing",19]
[null,"Description of Deficiency","X",null,"Critical Item Flag",20]
[null,"Action taken / required","Y",null,"Audit Type",21]
[null,"PO ref no","Z"]
[null,"Date completed","AA"]

{"sheet":"Ship_information","index":19,"n_rows":2,"n_cols":4,"rows_kept":2,"cut":false,"hidden":true,"merged":[]}
["Ship_ID","Ship_Name","FILE_NAME","Export_Date"]
["45","DHT SCANDINAVIA (08-01-2024)","45_1704686615391.xlsm","2024-07-05 12:07:80"]

{"sheet":"External_Deficiency_type","index":20,"n_rows":5,"n_cols":3,"rows_kept":5,"cut":false,"hidden":true,"merged":[]}
["TITLE","Type of deficiency_description","ID"]
["Condn of Class / Memo",null,5]
["Defect",null,1]
["Non Conformity",null,2]
["Observation",null,3]

{"sheet":"External_Inspection_type","index":21,"n_rows":11,"n_cols":2,"rows_kept":11,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Cargo Audit",17]
["Flag State Insp.",5]
["ISM Audit",2]
["ISPS Audit",3]
["MLC Audit",1]
["Nav Audit / Verification",8]
["OM Insp. (Eg. SIRE / CDI etc.)",6]
["Others (Eg. Insurance etc.)",12]
["PSC Inspection",4]
["Terminal Insp.",11]

{"sheet":"External_Observer_code","index":22,"n_rows":7,"n_cols":3,"rows_kept":7,"cut":false,"hidden":true,"merged":[]}
["TITLE","Observer_code_description","ID"]
["Class Surveyor",null,4]
["FSC Inspector",null,5]
["Others (Eg. Insurance etc.)",null,9]
["PSC Insp.",null,6]
["SIRE / CDI Insp.",null,8]
["Terminal Insp.",null,7]

{"sheet":"Sheet Version","index":23,"n_rows":2,"n_cols":2,"rows_kept":2,"cut":false,"hidden":true,"merged":[]}
["Version","Title"]
["2.0","Version 2.0"]