{"text_format":"1","workbook":"xlsx","n_sheets":24,"sheets":["Mainsheet","Completed","Calc","Areaofobs","Vessel_type","Deficiency_type","VIQrefno","Equipment_list","PSC_MOU","Inspection_type","Deficiency_Cause","Observer_code","Status_code","PSC_ref_no","Risk_value_of_obs","Year","Month","Date_","Sheet1","Ship_information","External_Deficiency_type","External_Inspection_type","External_Observer_code","Sheet Version"],"not_rendered":{"charts":0,"images":1,"macros":1,"external_links":0,"defined_names":12,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Mainsheet","index":0,"n_rows":62,"n_cols":28,"rows_kept":62,"cut":false,"hidden":false,"merged":[[10,8,10,9],[10,12,10,13],[12,6,12,27],[8,6,8,27]]}
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,"Defect - Damage Monitoring Sheet"]
[]
[null,null,null,null,null,null,null,"Date of Report","30-Jul-2024",null,null,"Ship Name","DHT TAIGA (01-06-2024)"]
[]
[null,null,null,null,null,null,"VERSION : 2.0"]
[]
[]
[]
[null,null,null,"ID","SHIPSIDE UNIQUEID","UNIQUE ID","Date Recorded","Type of Deficiency","Observer code","Type of Inspection","Description of Deficiency","Equipment Categories","Area of Observation","Deficiency Cause","VIQ Ref Number","Risk Value of Obs","PSC Ref Number","PSC MOU ID","Action Taken or Required","Target Date","PO Ref No.","Status Code","Date Completed","Drydock","Info Sharing","Critical Item","Audit Type","Superintendent Remarks"]
[null,null,null,null,41446,"0_Fri May 24 2024 19:27:47 GMT+0800","2024-03-28T08:00:00","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","whrs system LP side 2 temperature sensors  faulty. To be renewed","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","TEMPERATURE SENSORS ORDERED. RECEIVED WROG SPARES. MESSAGE SENT AGAIN","2024-06-30T08:00:00","STAI245042","Waiting spare",null,"No","No","No","Internal","please mention the wrong supply RO from Alfa Laval.\ncorrect type spares query"]
[null,null,null,34448,47188,"48_Sun Mar 03 2024 08:56:01 GMT+0800","2024-03-29T23:59:35","Defect","Ship Staff","Ship Staff Insp.","THE PCB of BWTS Electrohydraulic valve no2212 (inlet to filter) defective and not responding.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.11","Medium","","","The defective PCB swapped with the bypass valve no.1213(bypass filter) and is found working satisfactory. Requisition raised for the PCB","2024-06-19T23:59:35","STAI240062","Waiting spare",null,"No","No","No","Internal","spare ready for connection at Corpus, complete upon receipt of spares\nAlso upgrade to NF type will be taken up soon this year"]
[null,null,null,35329,67805,"0_Fri May 24 2024 19:29:20 GMT+0800","2024-04-03T23:59:35","Defect","Ship Staff","Ship Staff Insp.","G.E. F.O VISCOSITY CONTROLLER SENSOR FAULT","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","RO RAISED  FOR SAME","2024-07-03T23:59:35","STAI240136","Waiting spare",null,"No","No","No","Internal","spares processed for supply at Corpus Christi"]
[null,null,null,null,26129,"0_Fri May 24 2024 19:37:11 GMT+0800","2024-04-16T08:00:00","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ME UNIT #5 WATER LEAK FROM LINER JACKET TO RECTIFY","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Leak rectified.","2024-07-15T08:00:00","","In progress","2024-07-11T08:00:00","No","No","No","Internal","the jacket is jacked from below and kept in place. holding screw to reinstall after removing the broken studs."]
[null,null,null,35330,79184,"0_Fri May 24 2024 19:44:22 GMT+0800","2024-04-16T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","GANGWAY TO IDENTIFY WORN OUT SHEAVES AND ARRANGE REPLACEMENT","Deck - Machinery","Structural Condn. / WT integrity ","Equipment Related","","","","","RO RAISED","2024-07-15T23:59:35","STAI240116","Waiting spare",null,"No","No","No","Internal","noted inspection completed in weekly report dated 26 May.\nspares to process"]
[null,null,null,null,61759,"0_Fri May 24 2024 19:47:08 GMT+0800","2024-04-16T08:00:00","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","#5P & #5 S WATER BALLAST TANKS ABOUT EIGHT ANODES TO INSTALL ON THE TOP TRINGER LEVEL AFT SIDE","Deck - Machinery","Cargo / Ballast Systems","Equipment Related","","","","","Ballast Tank Inspection carried out, found that anodes missing since the delivery of the vessel. No anodes found in 1W's - 4W's WBT, 5W's WBT around 10 anodes found fitted","2024-07-15T08:00:00","","Not Started","2024-07-26T08:00:00","No","No","No","Internal","anodes missing from new building. with vessel age need to add up. Raise Ro and include in ref column"]
[null,null,null,null,30715,"48_Sat Jun 01 2024 01:37:15 GMT+0800","2024-04-16T08:00:00","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Space heaters for two motors not working (ME Fuel booster pump no 2 and Boiler feed water pump no 1)","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","11.10","Medium","","","R.O Raised","2024-07-15T08:00:00","STAI 240102","Waiting spare",null,"No","No","No","Internal","spares processed , awaiting connection."]
[null,null,null,null,73458,"0_Fri May 24 2024 19:35:56 GMT+0800","2024-04-16T08:00:00","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","MGO CHILLER NOT IN USE, TO CHECK AND PUT IN USE EVERY TIME WITH LSMGO","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Changed oil for compressors. Found atht HMI panel not working.  RO raised for same.","2024-07-16T08:00:00","STAI240153","Waiting spare",null,"No","No","No","Internal","complete and close on priority"]
[null,null,null,35327,26431,"0_Fri May 24 2024 19:41:04 GMT+0800","2024-04-16T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ACCOMODATION GANGWAY ROLLERS BREAKING AWAY","Deck - Machinery","Structural Condn. / WT integrity ","Equipment Related","","","","","RO RAISED ","2024-07-15T23:59:35","STAI240116","Waiting spare",null,"No","No","No","Internal"]
[null,null,null,35334,48645,"0_Fri May 24 2024 19:48:26 GMT+0800","2024-05-15T23:59:35","Observation","Ship Staff","Ship Staff Insp.","BOTTOM TIGHTENING STUD FOR CENTRAL COOLER NO.1 IS WASTED","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","RO RAISED","2024-08-17T23:59:35","STAI240137","Waiting spare",null,"No","No","No","Internal","complete as planned and close out"]
[null,null,null,null,46298,"48_Fri May 24 2024 20:44:51 GMT+0800","2024-05-17T08:00:00","Defect","Ship Staff","Ship Staff Insp.","NO1. VACCUM PUMP FOR T/G IS SEIZED NOT MOVING","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Opened up pump. Cleaned the parts . Bearings changed.\nMotor overhauled.   Corro coat applied  on casing but still not developing sufficient vacuum,","2024-08-15T08:00:00","STAI240146","In progress",null,"No","No","No","Internal","consider priority and complete the job"]
[null,null,null,null,38347,"48_Mon Jun 17 2024 09:50:54 GMT+0800","2024-06-15T08:00:00","Breakdown","Ship Staff","Ship Staff Insp.","M/E no 1 Fuel pump had bodily leaks","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","M/E Fuel pump cut off as per procedure in the manual. To overhaul spare fuel pump and renew at next available opportunity.","2024-08-17T08:00:00","","Not Started",null,"No","No","No","Internal"]
[null,null,null,null,30556,"48_Fri Jun 28 2024 02:33:21 GMT+0800","2024-06-22T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Calibration of JW 3way valve as hunting too much","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Require loop calibrator same ordered. Upon receiving we shall try to calibrate.","2024-09-28T08:00:00","STAI240156","Waiting spare",null,"No","No","No","Internal"]
[null,null,null,null,95863,"48_Fri Jun 28 2024 22:04:06 GMT+0800","2024-06-16T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Intermediate high pressure pipe from ME fuel pump no 1 is leaking, presently blanked due to fuel pump cut off.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","M/E to be stopped and O-rings of intermediate high pressure pipe needs to be renewed.","2024-08-28T08:00:00","","Not Started",null,"No","No","No","Internal"]
[null,null,null,null,57140,"48_Fri Jun 28 2024 22:05:56 GMT+0800","2024-06-15T08:00:00","Defect","Ship Staff","Ship Staff Insp.","M/E no 2 unit Jacket water inlet to cylinder cover gasket leaking slightly","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Gasket to be replaced on engine stopped condition.","2024-08-28T08:00:00","","Not Started",null,"No","No","No","Internal"]
[null,null,null,null,24357,"48_Fri Jun 28 2024 22:09:53 GMT+0800","2024-06-16T08:00:00","Defect","Ship Staff","Ship Staff Insp.","ME Air cooler drain orifice both chocked same needs to be cleared at anchorage.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Orifice to be cleared when engine stopped.","2024-08-28T08:00:00","","Not Started",null,"No","No","No","Internal"]
[null,null,null,null,50635,"0_Fri Jun 28 2024 22:11:59 GMT+0800","2024-06-16T08:00:00","Defect","Ship Staff","Ship Staff Insp.","All units ME Scavenge door gasket is leaking and found hardened during inspections. Same to order and replaced.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Scavenge door gasket to be ordered and replaced","2024-09-30T08:00:00","STAI240167","Waiting spare",null,"No","No","No","Internal"]
[null,null,null,null,68873,"48_Tue Jul 02 2024 04:23:02 GMT+0800","2024-06-15T08:00:00","Defect","Ship Staff","Ship Staff Insp.","ME Air cooler drain orifice both chocked same needs to be cleared","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","To clear orifice when engine stopped","2024-08-22T08:00:00","","Not Started",null,"No","No","No","Internal"]
[null,null,null,null,44773,"48_Tue Jul 02 2024 04:25:53 GMT+0800","2024-06-15T08:00:00","Defect","Ship Staff","Ship Staff Insp.","M/E viscometer not operational and S/F alarm active","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Valve positioner ordered through STAI240135. Sensor to be cleaned when engine is stopped.","2024-09-25T08:00:00","STAI240135","Waiting spare",null,"No","No","No","Internal"]
[null,null,null,null,71026,"48_Tue Jul 02 2024 04:27:25 GMT+0800","2024-06-15T08:00:00","Defect","Ship Staff","Ship Staff Insp."," M/E L.O Autoback wash filter bypass opened up for cleaning and found mesh to be damaged.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","To order 50 micron mesh and renew","2024-09-25T08:00:00","STAI245041","Waiting spare",null,"No","No","No","Internal"]
[null,null,null,null,92128,"48_Tue Jul 02 2024 04:30:59 GMT+0800","2024-06-16T08:00:00","Defect","Ship Staff","Ship Staff Insp.","No1 Main DG unit no 3 and 6 exhaust temp sensor erratic because of faulty cable","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","To order cable and replace the same, temporarily repaired and at present no active alarms. Sapres ordered thorugh STAI240066","2024-09-12T08:00:00","STAI240066","Waiting spare",null,"No","No","No","Internal"]
[null,null,null,null,55528,"48_Tue Jul 02 2024 04:35:35 GMT+0800","2024-06-17T08:00:00","Defect","Ship Staff","Ship Staff Insp.","HP Circulating pump low flow alarm active with both pumps. Suspect standby pump NRV discharge valve not closing and water short circuting.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Vessel in possession of 1 no valve, and 1 no valve ordered through STAI240176","2024-09-25T08:00:00","STAI240176","Waiting spare",null,"No","No","No","Internal"]
[null,null,null,null,38323,"48_Tue Jul 02 2024 04:37:06 GMT+0800","2024-06-29T08:00:00","Defect","Ship Staff","Ship Staff Insp.","M/E Bypass Filter valves not holding.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","To order and renew valves. Valves ordered through STAI240176","2024-09-17T08:00:00","STAI245041, STAI240176","Waiting spare",null,"No","No","No","Internal"]
[null,null,null,null,23495,"48_Tue Jul 02 2024 04:39:11 GMT+0800","2024-06-15T08:00:00","Defect","Ship Staff","Ship Staff Insp.","TG vacuum pump flap valve found to be broke","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Valves received, same to be replaced in next stoppage","2024-09-25T08:00:00","","In progress",null,"No","No","No","Internal"]
[null,null,null,null,34369,"48_Tue Jul 02 2024 04:43:37 GMT+0800","2024-06-26T08:00:00","Defect","Ship Staff","Ship Staff Insp.","AE LO purifier Heater cannot maintain 90'c maintaining temp only 85'c. Steam valves not holding","E/R - Purifier","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Commenced job but could not carry out as steam valves not holding, to replace steam valves to enable physical cleaning. Valves in possession awaiting changeover to LSMGO to replace valve.","2024-09-30T08:00:00","","In progress",null,"No","No","No","Internal"]
[null,null,null,null,50052,"48_Tue Jul 02 2024 04:45:31 GMT+0800","2024-06-10T08:00:00","Defect","Ship Staff","Ship Staff Insp.","EGCS Jet Section SW inlet line to Jet section bottom line is having soft patch.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Pin hole temporarily arrested by soft patch, need to do permanent repair.","2024-09-27T08:00:00","","Not Started",null,"No","No","No","Internal"]
[null,null,null,null,83917,"48_Tue Jul 02 2024 04:47:01 GMT+0800","2024-06-26T08:00:00","Defect","Ship Staff","Ship Staff Insp.","EGCS Absorber water controller valve out of order","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","To troubleshoot and order spares.","2024-09-18T08:00:00","STAI240161","Waiting spare",null,"No","No","No","Internal"]
[null,null,null,null,26602,"48_Tue Jul 02 2024 04:48:43 GMT+0800","2024-06-27T08:00:00","Defect","Ship Staff","Ship Staff Insp."," EGCS Sea chest copper anode is fully wasted","E/R - Aux. Mach.","","Equipment Related","10.32","Very High","","","Awaiting spares for replacement.","2024-09-25T08:00:00","STAI240157","Waiting spare",null,"No","No","No","Internal"]
[null,null,null,null,22219,"48_Tue Jul 02 2024 04:51:38 GMT+0800","2024-06-09T08:00:00","Defect","Ship Staff","Ship Staff Insp."," Sewage Collection tank level gauge not operational, ","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Awaiting Spares STAI240152","2024-09-25T08:00:00","STAI240152","Waiting spare",null,"No","No","No","Internal"]
[null,null,null,null,90272,"0_Tue Jul 02 2024 04:52:53 GMT+0800","2024-06-16T08:00:00","Defect","Ship Staff","Ship Staff Insp."," Grey water pump not operational, impeller missing.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","To troubleshoot  and ask for spares.","2024-09-17T08:00:00","","Not Started",null,"No","No","No","Internal"]
[null,null,null,null,23295,"48_Tue Jul 02 2024 04:55:01 GMT+0800","2024-06-18T08:00:00","Defect","Ship Staff","Ship Staff Insp.","STP one no discharge pump valve not holding","E/R - Pipes/ valves & fittings,E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Awaiting spares to rectify","2024-09-23T08:00:00","STAI240139","Waiting spare",null,"No","No","No","Internal"]
[null,null,null,null,25372,"0_Tue Jul 02 2024 04:58:49 GMT+0800","2024-06-26T08:00:00","Defect","Ship Staff","Ship Staff Insp.","MGPS anode for high sea chest copper reading is jumping","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","waiting spare for replacement","2024-09-25T08:00:00","STAI240042","Waiting spare",null,"No","No","No","Internal"]
[null,null,null,null,31691,"48_Tue Jul 02 2024 05:00:53 GMT+0800","2024-06-18T08:00:00","Defect","Ship Staff","Ship Staff Insp.","No 2 FWG distillate pump is leaking","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Distillate pump opened up and seal lapped. Spares ordered .","2024-09-17T08:00:00","STAI240162","Waiting spare",null,"No","No","No","Internal"]
[null,null,null,null,24830,"48_Tue Jul 02 2024 05:03:11 GMT+0800","2024-06-20T08:00:00","Defect","Ship Staff","Ship Staff Insp.","No.1 FWG jacket water outlet butterfly valve found seized and left in open position so FWG will heat up when not in use as well.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","During ME stoppage need to check valve and replace the same. Pipeline to remove to renew valve.","2024-09-12T08:00:00","STAI240176","Waiting spare",null,"No","No","No","Internal"]
[null,null,null,null,73025,"48_Tue Jul 02 2024 05:10:17 GMT+0800","2024-06-20T08:00:00","Defect","Ship Staff","Ship Staff Insp.","ICO lube is giving 440 volt low insulation and in other forest series Isolation transformer has been installed to overcome the same","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","To check if isolation transformer supplied or will be supplied by office. Mail sent to office and auto elesupport intends to supply transformer.","2024-09-24T08:00:00","","In progress",null,"No","No","No","Internal"]
[null,null,null,null,45726,"48_Tue Jul 02 2024 05:13:46 GMT+0800","2024-06-27T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Galley Hot plate is giving low insulation","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Hot plate spares are requested through STAI240160.","2024-09-18T08:00:00","STAI240160","Waiting spare",null,"No","No","No","Internal"]
[null,null,null,null,88083,"48_Tue Jul 02 2024 05:15:20 GMT+0800","2024-06-20T08:00:00","Defect","Ship Staff","Ship Staff Insp.","ER Atmospheric Oil mist detection system which is an additional installation installed on forest series. 1 detector is faulty same isolated","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","spares requested through STAI240071","2024-09-26T08:00:00","STAI240071","Waiting spare",null,"No","No","No","Internal"]
[null,null,null,null,43745,"0_Tue Jul 02 2024 23:11:27 GMT+0800","2024-06-18T08:00:00","Observation","Ship Staff","Ship Staff Insp.","Cosmetic upgradation of the fwd mooring winches / windlass to be taken","Deck - Mooring Machinery","Mooring","Equipment Related","9.15","Medium","","","Cosmetic upgradation of the fwd mooring winches / windlass in Progress","2024-09-18T08:00:00","","In progress",null,"No","No","No","Internal"]
[null,null,null,null,10674,"0_Tue Jul 02 2024 23:14:39 GMT+0800","2024-06-18T08:00:00","Observation","Ship Staff","Ship Staff Insp.","Cosmetic upgradation of main deck and associated pipelines, supports and fittings","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.5","Medium","","","In Progress","2024-09-18T08:00:00","","In progress",null,"No","No","No","Internal"]
[null,null,null,null,56755,"0_Tue Jul 02 2024 23:20:57 GMT+0800","2024-06-18T08:00:00","Observation","Ship Staff","Ship Staff Insp.","Midship hose handling crane de rusting and painting required","Deck - Machinery","General Appearance","Equipment Related","11.8","Low","","","De-rusting and painting to be taken","2024-09-18T08:00:00","","In progress",null,"No","No","No","Internal"]
[null,null,null,null,70110,"0_Tue Jul 02 2024 23:41:02 GMT+0800","2024-06-18T08:00:00","Observation","Ship Staff","Ship Staff Insp.","Forward stbd breast winch bollard off no 13 chock has its stopper securing eye broken/dislodged from the weld. This bollard is required during STS operation","Deck - Mooring Machinery","Mooring","Equipment Related","8.77","Medium","","","Welding of this eye to be taken in due course after meeting the gas freeing requirement and office concurrence for hot work","2024-09-18T08:00:00","","Not Started",null,"No","No","No","Internal"]
[null,null,null,null,26982,"48_Sun Jul 28 2024 12:53:26 GMT+0800","2024-07-26T08:00:00","Defect","Ship Staff","Ship Staff Insp.","OWS bilgemon battery low and Bilgeguard fuse blown","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","6.12","Medium","","","We have managed to get the bilgeguard display on with fuse. but we have about 30 minutes time difference with Bilgemon 488. we have received spare Bilgemon 488 as well.Mailed office if it needs to be repalced.","2024-08-08T08:00:00","STAI245053, STAI245055","In progress",null,"No","No","No","Internal"]
[null,null,null,null,21961,"48_Sun Jul 28 2024 13:01:51 GMT+0800","2024-07-27T08:00:00","Defect","Ship Staff","Ship Staff Insp.","COPT no 3 spring grease pot cover broken","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Temporarily rectified but need to order spares.","2024-09-28T08:00:00","","In progress",null,"No","No","No","Internal"]
[null,null,null,null,83137,"48_Sun Jul 28 2024 13:03:58 GMT+0800","2024-07-28T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Vaccum pump ammeter full load current red needle broken and fall within ammeter","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","to order and renew ammeter","2024-10-25T08:00:00","","Not Started",null,"No","No","No","Internal"]
[null,null,null,null,22214,"48_Mon Jul 29 2024 17:03:28 GMT+0800","2024-07-28T08:00:00","Defect","Ship Staff","Ship Staff Insp.","AE L.O storage tank level has S/F alarm active","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Troubleshooting revealed composition type pneumatic modulation unit problem,, same to be ordered.","2024-09-29T08:00:00","","Waiting spare",null,"No","No","No","Internal"]

{"sheet":"Completed","index":1,"n_rows":663,"n_cols":28,"rows_kept":663,"cut":false,"hidden":false,"merged":[[10,8,10,9],[10,12,10,13],[12,6,12,27],[8,6,8,27]]}
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,"Defect - Damage Monitoring Sheet"]
[]
[null,null,null,null,null,null,null,"Date of Report","30-Jul-2024",null,null,"Ship Name","DHT TAIGA (01-06-2024)"]
[]
[null,null,null,null,null,null,"VERSION : 2.0"]
[]
[]
[]
[null,null,null,"ID","SHIPSIDE UNIQUEID","UNIQUE ID","Date Recorded","Type of Deficiency","Observer code","Type of Inspection","Description of Deficiency","Equipment Categories","Area of Observation","Deficiency Cause","VIQ Ref Number","Risk Value of Obs","PSC Ref Number","PSC MOU ID","Action Taken or Required","Target Date","PO Ref No.","Status Code","Date Completed","Drydock","Info Sharing","Critical Item","Audit Type","Superintendent Remarks"]
[null,null,null,6226,null,"48_24/10/2019 9:47:45 PM","2018-12-26T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Anemometer- Wind speed transmitter found not working","Navigation - Others","Navigation","Equipment Related","4.7","High","","","Old repaired Anemometer transmitter installed. Tested and found operational.","2019-01-05T23:59:35","","Completed","2019-01-04T23:59:35","No","No","No","Internal"]
[null,null,null,6227,null,"48_24/10/2019 9:52:15 PM","2019-01-02T23:59:35","Defect","Ship Staff","Ship Staff Insp.","FWD air horn non operational","Navigation - Others","Navigation","Equipment Related","10.37","Medium","","","Air horn compressor and motor overhauled , fitted back and tried out, working satisfactory.","2019-01-09T23:59:35","","Completed","2019-01-09T23:59:35","No","No","No","Internal"]
[null,null,null,6228,null,"48_24/10/2019 9:57:34 PM","2019-01-03T23:59:35","Defect","Ship Staff","Ship Staff Insp.","IG Fan drain line in 3rd deck platform found leaking due to crack in the pipeline.","Inert Gas","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","New pipe fabricated wid stainless steel pipe and flange . Pipe replaced with fabricated one and tested, found satisfactory.","2019-01-03T23:59:35","","Completed","2019-01-03T23:59:35","No","No","No","Internal"]
[null,null,null,6229,null,"48_24/10/2019 9:59:53 PM","2019-01-03T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Main engine unit no.4 cyl.jacket inlet pipe leaking from flange joint.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Gasket replaced and boxed back with stainless steel bolts.","2019-01-07T23:59:35","","Completed","2019-01-07T23:59:35","No","No","No","Internal"]
[null,null,null,6230,null,"48_24/10/2019 10:02:27 PM","2019-01-05T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Hydraulic oil leakage from FWD windlass (PORT) High/Low control lever (DIRECTIONAL CONTROL VALVE)","Deck - Machinery","Mooring","Equipment Related","9.2","Very High","","","Both seals and o rings changed for the Directional control valve andf tested, and found working satisfactory.","2019-01-09T23:59:35","","Completed","2019-01-09T23:59:35","No","No","No","Internal"]
[null,null,null,6160,null,"48_24/10/2019 10:38:50 PM","2019-01-19T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Main deck port side,U - Clamps on hydraulic lines, FW lines and air lines found rusted.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related,External Factors","11.5","Medium","","","All rusts removed and painted.","2019-04-19T23:59:35","","Completed","2019-02-17T23:59:35","No","No","No","Internal"]
[null,null,null,6161,null,"48_24/10/2019 10:41:44 PM","2019-01-19T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","SIP'S around the accommodation not clearly marked.","Hull & Tanks","General Appearance","External Factors,Human Error","11.6","Medium","","","SIP markings completed.","2019-04-19T23:59:35","","Completed","2019-02-20T23:59:35","No","No","No","Internal"]
[null,null,null,6162,null,"48_24/10/2019 10:43:36 PM","2019-01-19T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ME UNIT # 6 Starting air valve solenoid cable was reported damaged, junction box found open and new cable laid externally, cable to be routed properly.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Cable renewed.","2019-04-19T23:59:35","","Completed","2019-03-02T23:59:35","No","No","No","Internal"]
[null,null,null,6163,null,"48_24/10/2019 10:46:03 PM","2019-01-19T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Mooring wires dry and rusty not greased using wire rope greaser.","Deck - Machinery,Deck - Mooring Machinery","Mooring","Equipment Related,Human Error","9.17","High","","","All mooring wires greasing carried out.","2019-04-19T23:59:35","","Completed","2019-03-13T23:59:35","No","No","No","Internal"]
[null,null,null,6164,null,"48_24/10/2019 10:48:36 PM","2019-01-19T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Port MGPS CU-AL anode showing error.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.37","Medium","","","Defective control PCB for CU and AL-Anode replaced with new spare Port MGPS is operational.","2019-04-19T23:59:35","","Completed","2019-04-13T23:59:35","No","No","No","Internal"]
[null,null,null,6165,null,"48_24/10/2019 10:50:32 PM","2019-01-19T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Dead man alarm indication light in pump room entrance not operational.","Elect. Mach. & Equip.","Cargo / Ballast Systems","Equipment Related","11.11","Very High","","","Received spare. Modified the switch and fitted back. It is working now.","2019-10-22T23:59:35","","Completed","2019-08-31T23:59:35","No","No","No","Internal"]
[null,null,null,6231,null,"48_24/10/2019 10:06:01 PM","2019-01-19T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","COPT # 2 Discharge line flange valve no.260 in pump room found traces of oil leakage.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.44","High","","","Oil traces cleaned and flange tightened,no oil leakage","2019-04-19T23:59:35","","Completed","2019-01-22T23:59:35","No","No","No","Internal"]
[null,null,null,6232,null,"48_24/10/2019 10:11:45 PM","2019-01-19T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Stenciling of various remote sounding boxes for ballast tanks missing","Hull & Tanks","General Appearance","Human Error","11.7","High","","","Steciling carried out for all remote sounding boxes for ballast tanks","2019-04-19T23:59:35","","Completed","2019-01-20T23:59:35","No","No","No","Internal"]
[null,null,null,6233,null,"48_24/10/2019 10:14:28 PM","2019-01-19T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","One light in pump room 2nd deck not working.","Elect. Mach. & Equip.","Cargo / Ballast Systems","Equipment Related","11.11","Very High","","","Light renewed","2019-01-19T23:59:35","","Completed","2019-01-20T23:59:35","No","No","No","Internal"]
[null,null,null,6234,null,"48_24/10/2019 10:17:16 PM","2019-01-19T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Pressure regulator in air line for sea chest testing not fitted","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related,Human Error","6.4","High","","","Pressure regulator fitted in air line for sea chest testing.","2019-04-19T23:59:35","","Completed","2019-02-03T23:59:35","No","No","No","Internal"]
[null,null,null,6235,null,"48_24/10/2019 10:19:29 PM","2019-01-19T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Windlass pinion bearing found not greased and grease point not clearly marked.","Deck - Machinery,Deck - Mooring Machinery","Mooring","Equipment Related,Human Error","9.2","Very High","","","Windlass pinion bearing greasing carried out and grease point marked.","2019-04-19T23:59:35","","Completed","2019-01-28T23:59:35","No","No","No","Internal"]
[null,null,null,6236,null,"48_24/10/2019 10:24:15 PM","2019-01-19T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Helicopter equipement CO2 extinguishers not as per requirement","LSA / FFA","Safety / LSA / FFA","Human Error,Knowledge Based","5.4","High","","","CO2 extinguishers installed as per requirement.","2019-04-19T23:59:35","","Completed","2019-02-02T23:59:35","No","No","No","Internal"]
[null,null,null,6237,null,"48_24/10/2019 10:26:52 PM","2019-01-19T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ME UNIT # 3 Starting air valve solenoid cable was reported damaged, junction box found open and new cable laid externally, cable to be routed properly.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related,Inappropriate Procedure","10.32","Very High","","","Cable renewed soon after receiving new cable.","2019-04-19T23:59:35","","Completed","2019-01-25T23:59:35","No","No","No","Internal"]
[null,null,null,6238,null,"48_24/10/2019 10:29:52 PM","2019-01-19T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","EGB bellow between LP and HP evaporator had traces of leakage, to be checked , cleaned and painted.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Bellow inspected, no leakes found.Bellow area cleaned and painted.","2019-04-19T23:59:35","","Completed","2019-02-08T23:59:35","No","No","No","Internal"]
[null,null,null,6166,null,"48_24/10/2019 10:59:49 PM","2019-01-21T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Port Side ECDIS unit on Bridge Buzzer for alarm is not working.","Elect. Mach. & Equip.","Navigation","Equipment Related","11.1","High","","","Replaced operation circuit for ECDIS 2 (part No. OPU CCK-976 (PC640,7PCRD1796B)). Buzzer working satisfactorily.","2019-10-22T23:59:35","","Completed","2019-08-25T23:59:35","No","No","No","Internal"]
[null,null,null,6167,null,"48_24/10/2019 11:05:55 PM","2019-01-28T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Main engine # 6 unit jacket water outlet temperature reading shows erratic","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Temperature sensor renewed and working satisfactory.","2019-01-28T23:59:35","","Completed","2019-01-28T23:59:35","No","No","No","Internal"]
[null,null,null,6168,null,"48_24/10/2019 11:07:47 PM","2019-02-07T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Vacuum toilet system port side line in operational","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Vacuum toilet line - Port side blockage rectified by flushing with water and air","2019-02-07T23:59:35","","Completed","2019-02-07T23:59:35","No","No","No","Internal"]
[null,null,null,6169,null,"48_24/10/2019 11:09:56 PM","2019-02-09T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Sewage overboard valve - minor leakage ( 2/3 drop/day) through the storm valve body at the Engine room bottom floor on port side","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Temporary measures have been taken with UW and normal steel putty and currently no sign of leakage. New valve has been ordered. In order to renew the valve plugging of Overboard line is required.Sewage overboard valve renewed at Singapore anchorage.","2019-05-22T23:59:35","","Completed","2019-05-12T23:59:35","No","No","No","Internal"]
[null,null,null,6170,null,"48_24/10/2019 11:11:49 PM","2019-02-12T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Main CSW pump no.1 - Discharge pressure gauge showing incorrect value","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Root valve for the pressure gauge renewed and line blown through - Gauge is operational.","2019-02-13T23:59:35","","Completed","2019-02-12T23:59:35","No","No","No","Internal"]
[null,null,null,6171,null,"48_24/10/2019 11:38:34 PM","2019-02-20T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Fresh water generator 1- Ejector pump sea water suction valve not holding, unable to isolate the pump.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","valve Renewed","2019-10-06T23:59:35","","Completed","2019-10-22T23:59:35","No","No","No","Internal"]
[null,null,null,6172,null,"48_24/10/2019 11:42:28 PM","2019-02-21T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Citadel Iridium Phone displaying \"SIM Card Blocked\" and can't be used.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","7.6","Medium","","","Troubleshooting carried out with the help of IT departments. Phone is operational now.","2019-03-11T23:59:35","","Completed","2019-03-22T23:59:35","No","No","No","Internal"]
[null,null,null,6173,null,"48_24/10/2019 11:47:00 PM","2019-02-26T23:59:35","Defect","Ship Staff","Ship Staff Insp.","ME Jacket pre heater steam inlet pressure gauge needle found broken.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Pressure gauge renewed.","2019-02-26T23:59:35","","Completed","2019-02-27T23:59:35","No","No","No","Internal"]
[null,null,null,6174,null,"48_24/10/2019 11:49:58 PM","2019-03-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","ME- Aft Aux. Blower cooling fan blades found damaged","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","ME- Aft Aux. Blower cooling fan renewed and tested.","2019-03-01T23:59:35","","Completed","2019-03-02T23:59:35","No","No","No","Internal"]
[null,null,null,6175,null,"48_25/10/2019 8:39:58 AM","2019-03-15T23:59:35","Defect","Ship Staff","Ship Staff Insp.","TG condenser –Condensate water inlet to vapour chamber pressure gauge found faulty","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Pressure gauge renewed.","2019-03-15T23:59:35","","Completed","2019-03-15T23:59:35","No","No","No","Internal"]
[null,null,null,6176,null,"48_25/10/2019 8:54:11 AM","2019-03-17T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Main Engine -Fuel oil Viscotherm is showing erratic reading.","Elect. Mach. & Equip.,E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.37","Medium","","","Sensor received and changed. Showing viscosity correctly","2019-06-16T23:59:35","","Completed","2019-07-01T23:59:35","No","No","No","Internal"]
[null,null,null,6177,null,"48_25/10/2019 8:56:53 AM","2019-03-18T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Auxiliary Engine - T/C Exhaust gas inlet temperature sensor -A found faulty","E/R - Aux. Engine,Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.37","Medium","","","Sensor renewed and is operational.","2019-03-19T23:59:35","","Completed","2019-03-18T23:59:35","No","No","No","Internal"]
[null,null,null,6178,null,"48_25/10/2019 8:59:47 AM","2019-03-20T23:59:35","Defect","Ship Staff","Ship Staff Insp.","WBT 3 (P) and WBT 5 (P) gauges showing erratic reading","Hull & Tanks","Cargo / Ballast Systems","Equipment Related","8.8","Medium","","","5P & 3P WBT sensor renewed.","2019-10-22T23:59:35","","Completed","2019-09-22T23:59:35","No","No","No","Internal"]
[null,null,null,6179,null,"48_25/10/2019 9:01:57 AM","2019-03-23T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Port windlass brake cylinder top cover seal slightly leaking","Deck - Machinery,Deck - Mooring Machinery","Mooring","Equipment Related","9.2","Very High","","","Scraper ring, wear ring and rod seal renewed for top cover and tested - working satisfactory.","2019-03-24T23:59:35","","Completed","2019-03-23T23:59:35","No","No","No","Internal"]
[null,null,null,8610,null,"48_Thu Sep 12 2019 17:50:29 GMT+0000 (Coordinated Universal Time)","2019-04-02T23:59:35","Defect","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","No evidence when the workshop and upper deck oxylacy regulators were last inspected annually or renewed in the last 5 years.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Inappropriate Procedure","5.26","Medium","","","New regulators for Oxygen and Acetylene were\n\nordered and were received by the vessel on 19th April 2019 at Singapore and the regulators\n\nwere replaced the same day.\n\nAll the documentation regarding the renewal of these regulators has been filed on board for\n\nrecords. Additionally the job for annual inspection and five yearly renewal of these regulators\n\nhas been added in the PMS for proper record keeping.","2019-04-17T23:59:35","","Completed","2019-04-10T23:59:35","No","No","No","External"]
[null,null,null,6180,null,"48_25/10/2019 9:03:51 AM","2019-04-07T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Pump Room Blower Motor Low Insulation.","Deck - Machinery,Elect. Mach. & Equip.","Cargo / Ballast Systems","Equipment Related","10.38","Medium","","","Pump Room fan motor inside the terminal box one wire connection to motor winding got grounded, same replaced with new wire and motor both bearing changed with new spare, blower is operational","2019-04-19T23:59:35","","Completed","2019-04-15T23:59:35","No","No","No","Internal"]
[null,null,null,6181,null,"48_25/10/2019 9:07:39 AM","2019-04-19T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Forward whistle horn , reported not working","Elect. Mach. & Equip.","Navigation","Equipment Related","11.1","High","","","Motor electrical connection disconnected to facilitate the repair work of the whistle. Complete unit removed from its place and taken to workshop. Dismantled the unit and found connecting rod bearing completely damaged. Same replaced with old","2019-04-20T23:59:35","","Completed","2019-04-20T23:59:35","No","No","No","Internal"]
[null,null,null,8601,null,"48_Mon Dec 09 2019 23:18:36 GMT+0000 (Coordinated Universal Time)","2019-04-21T23:59:35","Defect","Ship Staff","Nav Audit / Verification","Course Recorder was not marked and entries made after every Navigation watch.","Documentation","Navigation","Human Error","4.7","High","","","Missed entry was entered by concerned officer. Officer briefed regarding same. All officers briefed regarding the importance of making appropriate entries in log books and other records prior handing over watch so as to prevent recurrence.","2019-05-06T23:59:35","","Completed","2019-04-24T23:59:35","No","No","No","Internal"]
[null,null,null,8602,null,"48_Thu Sep 12 2019 23:21:55 GMT+0000 (Coordinated Universal Time)","2019-04-21T23:59:35","Defect","Ship Staff","Nav Audit / Verification","1 ENC Permit in ECDIS not updated.","Navigation - ECDIS","Navigation","External Factors","4.12","Very High","","","Navtor informed regarding missing ENC update and assistance requested to recify same. All permits received and uploaded in ECDIS system. All ECDIS ENC permits  updated to latest corrections. All were briefed : All officers to be well conversant with ECDIS and Navtor so as to ensure when receiving and updating ECDIS, all ENC permits are updated till latest week. Any missing update to be immediately reported to Navtor for rectifing same.","2019-05-06T23:59:35","","Completed","2019-04-21T23:59:35","No","No","No","Internal"]
[null,null,null,8603,null,"48_Mon Dec 09 2019 23:26:04 GMT+0000 (Coordinated Universal Time)","2019-04-21T23:59:35","Defect","Ship Staff","Nav Audit / Verification","No.2 ECDIS (Backup) Audible alarm not working.","Navigation - ECDIS","Navigation","Equipment Related","4.7","High","","","All officers informed regarding inoperational audible alarm on No.2 ECDIS. No.1 ECDIS alarm checked and found working satisfactory. Office informed regarding same and assistance requested to rectify the faulty audible alarm. Attended by maker's technician and issue resolved.","2019-06-21T23:59:35","","Completed","2019-05-12T23:59:35","No","No","No","Internal"]
[null,null,null,6182,null,"48_25/10/2019 9:09:58 AM","2019-04-22T23:59:35","Defect","Ship Staff","Ship Staff Insp.","CONNING DISPLAY ,PROCESSOR FAN FAIL","E/R - Aux. Mach.,Navigation - Others","Eng. / Strg. Comp.","Equipment Related","11.1","High","","","processor fan replaced by CODAR technician at Singapore","2019-07-23T23:59:35","STAI190081","Completed","2019-05-12T23:59:35","No","No","No","Internal"]
[null,null,null,8596,null,"48_Mon Dec 09 2019 18:06:28 GMT+0000 (Coordinated Universal Time)","2019-04-26T23:59:35","Defect","PSC Insp.","PSC Inspection","A Steam return pipe connection in work shop leaking","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Human Error","11.4","Very High","Other","","Cargo discharge stopped and steam line de-pressurised and isolated. Leaking flange gasket renewed and leak rectified / tested. Vessel resumed heating of slop tanks and Discharge operations","2019-04-26T23:59:35","","Completed","2019-04-26T23:59:35","No","No","No","External"]
[null,null,null,8597,null,"48_Mon Dec 09 2019 18:09:46 GMT+0000 (Coordinated Universal Time)","2019-04-26T23:59:35","Defect","PSC Insp.","PSC Inspection","The operating direction mark for ventilator of steering gear room not visible.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Human Error","11.6","Medium","Water/Weathertight condition","","Operating direction mark for ventilator was repainted immediately and PSC inspector verified same. ","2019-04-27T23:59:35","","Completed","2019-04-26T23:59:35","No","No","No","External"]
[null,null,null,6183,null,"48_25/10/2019 8:16:31 AM","2019-05-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Aux Boiler F.O. pump supply Mechanical seal leaking","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Mechanical Seal changed , P/P tried out satisfactory","2019-08-22T23:59:35","","Completed","2019-07-17T23:59:35","No","No","No","Internal"]
[null,null,null,6184,null,"48_25/10/2019 11:38:10 AM","2019-05-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Frequency controllers for MSW pumps #3 not working","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.37","Medium","","","FREQUENCY CONTROLLER FOR NO1 AND 2 ATTENDED ON 15/06/2019 AND NOW WORKING SATISFACTORY, As per office instructions Frequency controller not to be changed. Pump to","2019-08-21T23:59:35","","Completed","2019-06-06T23:59:35","No","No","No","Internal"]
[null,null,null,6185,null,"48_25/10/2019 11:41:49 AM","2019-05-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","VACUUMARATOR PUMP NO.1 END PLATE BADLY WORN OUT .","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Pump working satisfactory. Parts kept as spare. To be changed if issue arises","2019-08-16T23:59:35","","Completed","2019-06-28T23:59:35","No","No","No","Internal"]
[null,null,null,6186,null,"48_25/10/2019 11:45:20 AM","2019-05-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","IGS ECR Main control valve leaking when IG is venting to atmosphere and main blower in use","Inert Gas","Cargo / Ballast Systems","Equipment Related","10.32","Very High","","","Valve seat renewed. Tried out . No leakage observed","2019-08-21T23:59:35","STAI 190078","Completed","2019-07-27T23:59:35","No","No","No","Internal"]
[null,null,null,6187,null,"48_25/10/2019 11:48:09 AM","2019-05-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","GE fuel line Pr regulating v/v 9k leaking","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Confirmed the operation during LSMGO and HFO. Found not leaking. Holdingnow. Under observation. Vessel received spare. Kept standby","2019-10-22T23:59:35","STAI190112","Completed","2019-08-11T23:59:35","No","No","No","Internal"]
[null,null,null,6224,null,"48_25/10/2019 12:03:13 AM","2019-05-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Aux Boiler Feed water pumps motor #1 and #3 cooling Fan damaged","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Received the spare and changed the cooling fan. ","2019-11-21T23:59:35","","Completed","2019-10-29T23:59:35","No","No","No","Internal"]
[null,null,null,6188,null,"48_25/10/2019 11:51:49 AM","2019-05-03T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Control air dryer #1 not working","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.37","Medium","","","Spares received and changed. Found working satisfactory.","2019-10-22T23:59:35","","Completed","2019-09-26T23:59:35","No","No","No","Internal"]
[null,null,null,35395,16260,"48_Sat May 25 2024 00:59:15 GMT+0800","2019-05-05T23:59:35","Non Conformity","PSC Insp.","PSC Inspection"," A STEAM RETRUN  PIPE CONNECTION IN WORKSHOP LEAKING","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Human Error","","","","","Cargo discharge stopped and steam line de-pressurised and isolated. Leaking flange gasket renewed and leak rectified / tested. Vessel resumed heating of slop tanks and Discharge operations.","2019-05-05T23:59:35","","Completed","2019-05-05T23:59:35","No","No","No","External"]
[null,null,null,35397,37991,"0_Sat May 25 2024 01:08:28 GMT+0800","2019-05-05T23:59:35","Non Conformity","PSC Insp.","PSC Inspection","THE OPERATING DIRECTION MARK FOR VENTILATOR OF STEERING GEAR ROOM NOT CLEARLY VISIBLE","Miscellaneous","General Appearance","Human Error","","","Other","","MARKING DONE FOR VENTILATOR WAS IMMEDIATELY PAINTED AND PSC INSPECTOR VERIFIED.","2019-05-05T23:59:35","","Completed","2019-05-05T23:59:35","No","No","No","External"]
[null,null,null,6189,null,"48_25/10/2019 11:54:11 AM","2019-05-12T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","No 1 boiler burner platform has steam / leakage. Looks like same is from steam regulating valve.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Gasket to be renewed.","2019-05-22T23:59:35","","Completed","2019-05-15T23:59:35","No","No","No","Internal"]
[null,null,null,6190,null,"48_25/10/2019 11:56:47 AM","2019-05-12T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Air bottles auto drain valve is kept shut. Same to be opened and all the crew to be advised accordingly.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","VALVES OPENED AND CREW ADVISED OF THE OPERATION","2019-05-19T23:59:35","","Completed","2019-05-13T23:59:35","No","No","No","Internal"]
[null,null,null,6191,null,"48_25/10/2019 12:00:28 PM","2019-05-12T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Area below the blower in steering Gear room needs to be cleaned.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Area cleaned and painted","2019-07-12T23:59:35","","Completed","2019-05-25T23:59:35","No","No","No","Internal"]
[null,null,null,6192,null,"48_25/10/2019 1:36:51 PM","2019-05-12T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","In steam line there is steam / water leak from dump bypass valve and air ejector steam inlet valve. To be rectified by closing main steam stop valve","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","gasket renewed","2019-07-12T23:59:35","","Completed","2019-05-21T23:59:35","No","No","No","Internal"]
[null,null,null,6193,null,"48_25/10/2019 1:40:19 PM","2019-05-12T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Provision compressor low pressure gauge to renew","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Pressure Gauge renewed","2019-06-12T23:59:35","","Completed","2019-05-24T23:59:35","No","No","No","Internal"]
[null,null,null,6194,null,"48_25/10/2019 1:44:14 PM","2019-05-12T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Port side bunker manifold pressure gauge to renew, as same showing wrong indication.","Deck - Pipe / Fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Pressure Gauge renewed","2019-06-12T23:59:35","","Completed","2019-05-21T23:59:35","No","No","No","Internal"]
[null,null,null,6195,null,"48_25/10/2019 1:50:47 PM","2019-05-12T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","All 3 Aft winches gear case relief valve spring is missing. To replace.","Deck - Machinery","Mooring","Equipment Related","9.14","Medium","","","Springs replaced.","2019-06-12T23:59:35","","Completed","2019-06-05T23:59:35","No","No","No","Internal"]
[null,null,null,6196,null,"48_25/10/2019 1:56:01 PM","2019-05-12T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Stbd side pump room blower motor top cover is temporarily repaired by cold work. New cover to fabricate and fit.","Deck - Machinery","Cargo / Ballast Systems","Equipment Related","10.32","Very High","","","Top cover brought in E/R workshop and fabricated","2019-06-12T23:59:35","","Completed","2019-06-06T23:59:35","No","No","No","Internal"]
[null,null,null,6197,null,"48_25/10/2019 2:07:01 PM","2019-05-12T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","T/C air intake room cleaning required.","Miscellaneous","Eng. / Strg. Comp.","Human Error","10.29","Medium","","","Gratings removed, chipped and painted.","2019-07-12T23:59:35","","Completed","2019-06-11T23:59:35","No","No","No","Internal"]
[null,null,null,6198,null,"48_25/10/2019 2:09:27 PM","2019-05-16T23:59:35","Defect","Ship Staff","Suptd. Insp.","COPT#2 Oil caution remark from shore analysis","Cargo Mach.,Deck - Machinery","Cargo / Ballast Systems","Equipment Related","10.7","Medium","","","COPT NO2 OIL SUMP, DRAINED CLEANED AND OIL RENEWED","2019-06-12T23:59:35","","Completed","2019-06-03T23:59:35","No","No","No","Internal"]
[null,null,null,6199,null,"48_25/10/2019 2:12:28 PM","2019-05-16T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Few buttons on MF/HF keypad not functioning . Also,few pins of flat cable connected to the Keypad PCB found damaged making the above mentioned keys inoperational.","Navigation - GMDSS & Communication","Navigation","Equipment Related","4.21","High","","","MF/HF equipment flat cable renewed and tested the GMDSS found working satisfactory.","2019-08-21T23:59:35","STAI195045","Completed","2019-07-09T23:59:35","No","No","No","Internal"]
[null,null,null,6200,null,"48_25/10/2019 2:15:59 PM","2019-05-18T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Soot blower # 3 of LP side is stuck. Not operating","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Soot Blower LP3 removed from place , soot blower was stuck badly, sealing air passage was choked completely, same made free and cleared. Soot blower fitted back in place and tried out , satisfactory","2019-06-21T23:59:35","","Completed","2019-06-20T23:59:35","No","No","No","Internal"]
[null,null,null,6201,null,"48_25/10/2019 2:18:03 PM","2019-05-18T23:59:35","Critical Equipment,Defect","Ship Staff","Ship Staff Insp.","Clutch lining of Vacuum pump of Emergency Fire Pump came off while trying out of the pump","Critical Equip.","Emgcy. Systems","Equipment Related","5.41","Very High","","","Clutch lining renewed with the spare recd , pump tried out, satisfactory","2019-08-21T23:59:35","","Completed","2019-07-17T23:59:35","No","No","No","Internal"]
[null,null,null,6202,null,"48_25/10/2019 2:21:26 PM","2019-05-20T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Vibscanner is not operational","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Received new vibscanner. ","2019-11-21T23:59:35","","Completed","2019-10-29T23:59:35","No","No","No","Internal"]
[null,null,null,6203,null,"48_25/10/2019 2:25:15 PM","2019-05-23T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Siren for wind Hi-Hi alarm not operational and only light is working.","Elect. Mach. & Equip.","Cargo / Ballast Systems","Equipment Related","10.37","Medium","","","Spares received at Singapore on 31/08/2019. Wind Hi-Hi siren and light replaced. Working satsifactorily","2019-10-22T23:59:35","","Completed","2019-08-24T23:59:35","No","No","No","Internal"]
[null,null,null,6204,null,"48_25/10/2019 2:29:07 PM","2019-06-02T23:59:35","Critical Equipment,Defect","Ship Staff","Ship Staff Insp.","The GMT time in the BilgeGuard is 11-12 minutes behind the actual GMT time","Critical Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","CHANGED 15 PPM MONITOR. NOW DIFFERENCE IS 3 MINS","2019-10-21T23:59:35","","Completed","2019-10-03T23:59:35","No","No","No","Internal"]
[null,null,null,6205,null,"48_25/10/2019 2:32:38 PM","2019-06-02T23:59:35","Defect","Ship Staff","Ship Staff Insp.","One of the Personal Gas Meter MSA Altair 4X (Sr no. 06028737) Showing Error message on O2, CO & H2S sensor on starting the equipment","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.23","Very High","","","Replaced with the new gas meter received under warranty at GOLA, US on 09th July 2019","2019-08-21T23:59:35","","Completed","2019-06-30T23:59:35","No","No","No","Internal"]
[null,null,null,6206,null,"48_25/10/2019 2:37:17 PM","2019-06-03T23:59:35","Defect","Ship Staff","Ship Staff Insp.","The WBT gas detection system function giving Fault 19 and 17. and is inoperable. FAULT (19) - “No custom setup, using default setup” comes and later after 15-20 seconds the FAULT(17) – “Analyzing unit no answer” shows.","Critical Equip.,Elect. Mach. & Equip.","Cargo / Ballast Systems","Equipment Related","5.22","High","","","Makers technician attanded vessel at GOLA, US on 08th July 2019. Troubleshooting done, necessary spares changed by technician and reconfiguration done.","2019-08-21T23:59:35","","Completed","2019-06-29T23:59:35","No","No","No","Internal"]
[null,null,null,6207,null,"48_25/10/2019 2:40:16 PM","2019-06-03T23:59:35","Defect","Ship Staff","Ship Staff Insp.","UTI (Sr. No. G17710) showing error message on start up indicating ‘’No msg’’.","Miscellaneous","Cargo / Ballast Systems","Equipment Related","8.12","Medium","","","Tape was unwinded to check for any damage and found tape damage at 60cm mark. Continuity test was done for the UTI to confirm the tape error.As per message from office as vessel have total 4 UTIs, so this faulty UTI to be landed ashore at next","2019-10-22T23:59:35","","Completed","2019-07-25T23:59:35","No","No","No","Internal"]
[null,null,null,6208,null,"48_25/10/2019 2:42:33 PM","2019-06-07T23:59:35","Defect","Ship Staff","Ship Staff Insp.","WBT 1 (P) gauge showing erratic reading","Elect. Mach. & Equip.","Cargo / Ballast Systems","Equipment Related","8.8","Medium","","","Renewed sensor on 02nd Oct 2019.","2019-10-22T23:59:35","","Completed","2019-09-23T23:59:35","No","No","No","Internal"]
[null,null,null,6225,null,"48_25/10/2019 2:44:53 PM","2019-06-11T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Kyma Engine Analyser defective","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Changed the cable connecting to computer by Technician","2019-11-21T23:59:35","","Completed","2019-10-22T23:59:35","No","No","No","Internal"]
[null,null,null,6209,null,"48_25/10/2019 2:47:46 PM","2019-06-12T23:59:35","Defect","Ship Staff","Ship Staff Insp.","The local touch panel of WHRS( EGB) does not operate with touch, however operational with mouse","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.37","Medium","","","The touch screen panel renewed","2019-11-21T23:59:35","","Completed","2019-10-11T23:59:35","No","No","No","Internal"]
[null,null,null,6210,null,"48_25/10/2019 2:56:36 PM","2019-06-15T23:59:35","Defect","Ship Staff","Ship Staff Insp.","HFO PFR P/P NO2 MAGNETIC COUPLING CASING HOLED","E/R - Purifier","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","CHANGED CAN OF THE COUPLING","2019-10-22T23:59:35","","Completed","2019-10-01T23:59:35","No","No","No","Internal"]
[null,null,null,6211,null,"48_25/10/2019 2:59:03 PM","2019-06-20T23:59:35","Defect","Ship Staff","Ship Staff Insp.","KW not matching with KWh meter reading and which leads to high SFOC, diff in % utilization of AEs.Actually KWHR is not for present KW","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.37","Medium","","","RESET THE KWH METER. NOW SHOWING VALUES CORRECTLY","2019-10-22T23:59:35","","Completed","2019-10-06T23:59:35","No","No","No","Internal"]
[null,null,null,6212,null,"48_25/10/2019 3:06:56 PM","2019-06-27T23:59:35","Defect","Ship Staff","Ship Staff Insp.","M/E F.O. leak off alarm not coming in the AMS","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Changed the Net DI 16. found alarm stilll there. Then found that in the tag in the AMS the switch had shifted to Man. Changed back to Auto. It is working fine. Changed it back to old NET DI16. Still it is functional.","2019-09-21T23:59:35","","Completed","2019-09-01T23:59:35","No","No","No","Internal"]
[null,null,null,6213,null,"48_25/10/2019 3:13:00 PM","2019-07-03T23:59:35","Defect","Ship Staff","Ship Staff Insp.","EGB exhasut gas outlet temperature probe giving wrong readings","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","needs replacement. Shall raise RO for same. Entered in DD defect list","2019-09-21T23:59:35","","Completed","2019-09-06T23:59:35","No","No","No","Internal"]
[null,null,null,6222,null,"48_25/10/2019 4:23:34 PM","2019-07-09T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Stbd windlass Hydraulic brake Cylinder leaking from Cylinder top seal during anchoring operations","Deck - Mooring Machinery","Mooring","Equipment Related","9.2","Very High","","","Road seal and scrapper ring renewed. Brake tried out and found satisfactory. No further leaks observed.","2019-08-21T23:59:35","","Completed","2019-08-17T23:59:35","No","No","No","Internal"]
[null,null,null,6223,null,"48_25/10/2019 4:26:54 PM","2019-07-11T23:59:35","Defect","Ship Staff","Ship Staff Insp.","IG 43 - deck isolation valave for the IG Line after the IG NRV was found to be leaking and not holding","Cargo Mach.,Inert Gas","Cargo / Ballast Systems","Equipment Related","8.25","Very High","","","IG 43 valve removed from location and found valve disc damaged. Valve disc was builded and put back in plce again. But still minor leak exist. RO raised for Valve disc and seat ring. Valve renewed.","2019-10-21T23:59:35","STAI190182","Completed","2019-10-16T23:59:35","No","No","No","Internal"]
[null,null,null,6214,null,"48_25/10/2019 3:24:54 PM","2019-07-14T23:59:35","Defect","Ship Staff","Ship Staff Insp.","UTI (Sr. No. G18578) Display becomes blurred everytime after 5-10 minutes of operation","Miscellaneous","Cargo / Ballast Systems","Equipment Related","8.12","Medium","","","Interchanged with the Display unit of UTI G17710 which was to be landed ashore as per message from office. Now UTI G 18578 is in good working order","2019-10-22T23:59:35","","Completed","2019-07-25T23:59:35","No","No","No","Internal"]
[null,null,null,6215,null,"48_25/10/2019 3:35:14 PM","2019-07-14T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Work shop AC OCR under rated ,getting tripped","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.37","Medium","","","Spares received and changed. Found working satisfactory.","2019-10-22T23:59:35","","Completed","2019-09-30T23:59:35","No","No","No","Internal"]
[null,null,null,6216,null,"48_25/10/2019 3:37:27 PM","2019-07-15T23:59:35","Defect","Ship Staff","Ship Staff Insp.","STBD life boat control circuit switch damaged","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.29","High","","","Requisition received at Singapore on 31/08/2019. Control circuit replaced. Working satisfactorily now.","2019-10-06T23:59:35","","Completed","2019-08-25T23:59:35","No","No","No","Internal"]
[null,null,null,6217,null,"48_25/10/2019 3:42:18 PM","2019-07-15T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Two wire programmable TX defective","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Spares received and changed. Found working satisfactory.","2019-10-21T23:59:35","","Completed","2019-09-17T23:59:35","No","No","No","Internal"]
[null,null,null,6218,null,"48_25/10/2019 3:48:02 PM","2019-07-16T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Scrubber p/p mech seal leaking","E/R - Aux. Mach.","Cargo / Ballast Systems","Equipment Related","10.31","Very High","","","Mechanical sal renewed. Pump tried out.","2019-08-06T23:59:35","","Completed","2019-07-30T23:59:35","No","No","No","Internal"]
[null,null,null,6219,null,"48_25/10/2019 3:50:01 PM","2019-07-30T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Cover for General Alarm switch on Port/Stbd boat deck broken","Elect. Mach. & Equip.,LSA / FFA","Safety / LSA / FFA","Equipment Related","10.37","Medium","","","Spares received and changed. Found working satisfactory.","2019-10-22T23:59:35","","Completed","2019-10-02T23:59:35","No","No","No","Internal"]
[null,null,null,6220,null,"48_25/10/2019 3:52:18 PM","2019-08-02T23:59:35","Critical Equipment","Ship Staff","Ship Staff Insp.","The battery for BilgeMon 488 for OWS showing voltage 0.330 V against the required value of 2.5","Critical Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","CHANGED 15 PPM SENSOR WITH NEW","2019-10-22T23:59:35","","Completed","2019-10-03T23:59:35","No","No","No","Internal"]
[null,null,null,6221,null,"48_25/10/2019 3:57:52 PM","2019-08-07T23:59:35","Critical Equipment,Defect","Ship Staff","Ship Staff Insp.","Fire and GS p/p 1 mech seal leaking","Critical Equip.","Eng. / Strg. Comp.","Equipment Related","10.31","Very High","","","Pump dismantled and overhauled, mech seal and bottom line brearing renewed","2019-08-21T23:59:35","","Completed","2019-08-14T23:59:35","No","No","No","Internal"]
[null,null,null,9498,null,"48_10/01/2020 6:35:07 AM","2019-08-31T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Nav Audit / Verification","The actual time of arrival to each waypoint was not mentioned in the way point sheet of the passage plan. The arrival times were recorded in the deck log book. ","Navigation - Others","Navigation","Inappropriate Procedure","","","","","Vessel has sterted writing the actual time of arrival to each waypoint in the way point sheet of the passage plan as well as recording in the deck log book. All the navigating officers have been familiarised with correct procedures of filling the passage plan waypoint sheet.","2019-11-27T23:59:35","","Completed","2019-11-27T23:59:35","No","No","No","Internal"]
[null,null,null,9499,null,"48_10/01/2020 7:39:39 AM","2019-08-31T23:59:35","Observation","Owner / Marine / Tech. Suptd.","ISM Audit","Some of the SOPEP gear items (Shovels, broom) were not marked with the 2 red bands as required by company procedures.","Miscellaneous","MARPOL Related","Inappropriate Procedure","","","","","Shovels, Brooms, Scoops etc which were not having red band were marked with red band as per company procedures. All other items cross checked and found bearing red bands on them. Uncontrolled copy of COMPANY PROCEDURES (12.02.12.00.00) Posted in SOPEP LOCKER for easy reference for ship staff.","2020-11-29T23:59:35","","Completed","2020-11-27T23:59:35","No","No","No","Internal"]
[null,null,null,8595,null,"48_Thu Sep 12 2019 17:43:26 GMT+0000 (Coordinated Universal Time)","2019-08-31T23:59:35","Defect","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","The port and Starboard side hose crane's booms were not fitted with\n\nangle indicator.","Deck - Machinery","General Appearance","Equipment Related","8.5","Very High","","","OPERATORS COMMENTS:\n\nWe wish to inform that the port and stbd side hose handling cranes have a SWL of 20T and this\n\nSWL applies for the full operational range corresponding to maximum and minimum operating\n\nradius / angles, i.e. minimum operating radius of 4.4 meter and maximum operating radius of\n\n20 meter. The crane booms cannot be elevated or lowered to angles greater or lower than the\n\nstated operating radius / angle as the maximum and minimum radius limit is limited /\n\nrestricted by the cylinder’s stroke ends.\n\nSince these hose handling cranes are provided with limit devices for safe operation and the\n\nSWL of the crane is applicable over the whole range, an angle indicator has not been provided\n\nfor the boom by the Crane Maker. Same has been confirmed by the Crane Maker’s.\n\nWe also wish to confirm that the operating radius and SWL is permanently marked on the\n\nboom of these cranes. For ready reference we have attached the relevant pages from the\n\nmaker’s manual of the ship’s hose handling crane.","2019-09-15T23:59:35","","Completed","2019-09-15T23:59:35","No","No","No","External"]
[null,null,null,8598,null,"48_Thu Sep 12 2019 18:25:54 GMT+0000 (Coordinated Universal Time)","2019-09-30T23:59:35","Defect","Owner / Marine / Tech. Suptd.","ISM Audit","Two EEBD pressure found less than 200 bar due inspection","LSA / FFA","Safety / LSA / FFA","Human Error","5.44","High","","","EEBD were refilled to 200 bar pressure. All EEBDS and BA sets were checked to ensure compliance. Concerned officer was briefed to deligently carry out weekly and monthly checks and ensure compliance at all times.","2019-10-06T23:59:35","","Completed","2019-09-30T23:59:35","No","No","No","Internal"]
[null,null,null,8599,null,"48_Thu Sep 12 2019 18:29:30 GMT+0000 (Coordinated Universal Time)","2019-09-30T23:59:35","Defect","Owner / Marine / Tech. Suptd.","MLC Audit","Crew messroom refrigerator door packing damaged and food items kept inside spoilt.","Accommodation","MLC Related","Equipment Related","11.13","Low","","","Door packing was renewed and confirmed door sealing properly. ","2019-10-22T23:59:35","","Completed","2019-10-06T23:59:35","No","No","No","Internal"]
[null,null,null,8600,null,"48_Thu Sep 12 2019 18:33:33 GMT+0000 (Coordinated Universal Time)","2019-09-30T23:59:35","Defect","Owner / Marine / Tech. Suptd.","ISPS Audit","Anchor Hawse pipe cover not secured. ","Deck - Machinery","ISPS Related","Behaviour Based","7.12","High","","","Hawse pipe covers put in place and secured. All personnel briefed regarding Security procedures to be followed and precautions to be taken. Importance of securing hawse pipe covers reiterated to all.","2019-10-06T23:59:35","","Completed","2019-09-30T23:59:35","No","No","No","Internal"]
[null,null,null,6147,null,"48_25/10/2019 3:59:57 PM","2019-10-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Grey water discharge pump not taking suction.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Grey water discharge Pump overhauled, mouth ring renewed with spare","2020-02-01T23:59:35","STAI190222","Completed","2020-02-21T23:59:35","No","No","No","Internal","Spares received now. Please complete job ASAP. Target date revised accordingly."]
[null,null,null,6148,null,"48_24/10/2019 11:58:45 PM","2019-10-05T23:59:35","Defect","Ship Staff","Ship Staff Insp.","CCTV -CAMERA NO: 2 (FWD) NOT WORKING , CAMERA NO: 3 ( FUNNEL DECK ) -ERRATIC","Miscellaneous","ISPS Related","Equipment Related","7.6","Medium","","","As per Office instructions Defect to be closed","2020-04-19T23:59:35","","Completed","2020-04-26T23:59:35","No","No","No","Internal","New CCTV installation to be carried out.  Remove the defect from list."]
[null,null,null,6244,null,"48_2019-03-11 07:06:56.000","2019-10-22T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","Fwd Air horn not working.","Navigation - Others","Navigation","Equipment Related","","","","","Spares received and renewed. Fog horn assembled and now in use","2019-11-21T23:59:35","","Completed","2019-11-02T23:59:35","No","No","No","Internal"]
[null,null,null,8594,null,"48_Mon Mar 11 2019 07:06:56 GMT+0000 (Coordinated Universal Time)","2019-10-22T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","Fwd Air horn not working.","Navigation - Others","Navigation","Equipment Related","4.7","High","","","Spares received and renewed. Fog horn assembled and now in use","2019-11-21T23:59:35","","Completed","2019-11-02T23:59:35","No","No","No","Internal"]
[null,null,null,6145,null,"48_2019-08-11 19:37:25.000","2019-10-27T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Left over pneumatic pipe of old BWTS system in steering gear room to remove","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","All old pneumatic pipes removed and terminated. ","2019-11-06T23:59:35","","Completed","2019-11-01T23:59:35","No","No","No","External"]
[null,null,null,6150,null,"48_2019-08-11 09:37:39.000","2019-10-27T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Mooring wires are covered with mud due to use in yard. Cleaning and greasing required.","Miscellaneous","Mooring","Equipment Related,External Factors","9.17","High","","","All mooring wires cleaned and greasing carried out. Reported in weekly manitenance report. (DHT Taiga - Deck maintenance Report (16th Dec 2019 - 22nd Dec 2019).xlsx)","2020-01-27T23:59:35","","Completed","2019-12-11T23:59:35","No","No","No","Internal"]
[null,null,null,6151,null,"48_2019-08-11 09:46:40.999","2019-10-27T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Ship Staff Insp.","Various tank domes of WBT and COT has rust weep marks. Derusting and painting required.","Deck - Pipe / Fittings","Cargo / Ballast Systems","External Factors","8.18","High","","","All WBT and COT tank domes derusted and painted with full coat of green paint. Required Stencilling done.","2020-02-21T23:59:35","","Completed","2020-02-16T23:59:35","No","No","No","Internal"]
[null,null,null,6152,null,"48_2019-08-11 10:25:48.000","2019-10-27T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","All the PV valves inspection date stencil to change.","Deck - Pipe / Fittings","General Appearance","Equipment Related","8.21","High","","","stencilling of overhauling date  done on all PV valve.","2019-11-21T23:59:35","","Completed","2019-11-02T23:59:35","No","No","No","Internal"]
[null,null,null,6153,null,"48_2019-08-11 10:29:34.000","2019-10-27T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Outside pump room Stbd side air valve leaking, To be renewed.","Deck - Pipe / Fittings","Eng. / Strg. Comp.","Equipment Related","11.4","Very High","","","air manifold valve  renewed.","2019-11-11T23:59:35","","Completed","2019-11-09T23:59:35","No","No","No","Internal"]
[null,null,null,6154,null,"48_2019-08-11 10:45:11.000","2019-10-27T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Fire line pipe in scrubber room, just above the main power panel vibrates a lot at higher RPM. More supports to be welded.","LSA / FFA","Eng. / Strg. Comp.","External Factors","11.5","Medium","","","Fitted extra supports for pipe lines","2019-11-11T23:59:35","","Completed","2019-11-11T23:59:35","No","No","No","Internal"]
[null,null,null,6155,null,"48_2019-08-11 19:49:28.000","2019-10-27T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","MSDS and PPE to place in BWTS room for neutralizing chemicals.","Cargo Mach.","Cargo / Ballast Systems","Inappropriate Procedure","10.32","Very High","","","MSDS AND PPE placed in location.","2019-11-06T23:59:35","","Completed","2019-11-01T23:59:35","No","No","No","External"]
[null,null,null,6156,null,"48_2019-11-08 19:51:48.999","2019-10-27T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Various electrical insulation mat in E/R and emergency DG room are deteriorated or salt soaked. To be renewed.","Miscellaneous","Eng. / Strg. Comp.","Inappropriate Procedure","11.11","Very High","","","Insulation mats replaced.","2019-11-05T23:59:35","","Completed","2019-11-20T23:59:35","No","No","No","External"]
[null,null,null,6157,null,"48_2019-11-08 20:02:45.000","2019-10-27T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Zebra stripe sticker to put in the newly installed low head pipe in  ER bottom platform","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","External Factors","10.32","Very High","","","Stickers placed in location.","2019-11-03T23:59:35","","Completed","2019-11-08T23:59:35","No","No","No","External"]
[null,null,null,6158,null,"48_2019-11-08 20:13:51.000","2019-10-27T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ME LO auto filter shaft seal leaking. To be renewed","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Seal renewed.","2019-12-11T23:59:35","","Completed","2019-12-04T23:59:35","No","No","No","External",""]
[null,null,null,6159,null,"48_2019-08-11 20:17:42.000","2019-10-27T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Economiser surrounding to clean and paint","Miscellaneous","Eng. / Strg. Comp.","External Factors","10.32","Very High","","","To be painted. Painting completed by 30th Dec 2019","2019-12-22T23:59:35","","Completed","2019-12-21T23:59:35","No","No","No","External","Target date revised in view of busy schedule of the vessel."]
[null,null,null,6239,null,"48_2019-08-11 19:41:53.000","2019-10-27T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Water cooler outside ECR not operational. Cooler Compressor not running.","Miscellaneous","General Appearance","Equipment Related","10.32","Very High","","","Leak rectified and cooler put in use","2019-11-06T23:59:35","","Completed","2019-10-31T23:59:35","No","No","No","Internal"]
[null,null,null,6240,null,"48_2019-11-08 19:58:10.999","2019-10-27T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","T/C suction room door not easy to open. To ease up and grease.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","DOOR EASED UP. ","2019-10-30T23:59:35","","Completed","2019-10-28T23:59:35","No","No","No","External"]
[null,null,null,6241,null,"48_2019-11-08 20:07:39.000","2019-10-27T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Steering gear room door self-closing mechanism needs to adjust as door remains in open condition.","Miscellaneous","Eng. / Strg. Comp.","Inappropriate Procedure","10.32","Very High","","","Door adjusted. ","2019-10-29T23:59:35","","Completed","2019-10-29T23:59:35","No","No","No","External"]
[null,null,null,6242,null,"48_2019-08-11 20:09:57.000","2019-10-27T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Chlorine dosing pump of STP was running but no liquid passing. To be purged and checked regularly.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Checked and purged. ","2019-10-27T23:59:35","","Completed","2019-10-27T23:59:35","No","No","No","External"]
[null,null,null,6243,null,"48_2019-11-08 10:42:57.000","2019-10-27T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Drain near both aft E/R blower are choked. To be cleared.","Miscellaneous","Structural Condn. / WT integrity ","External Factors","6.2","High","","","Drain line opened up for both blowers and cleared. ","2019-11-26T23:59:35","","Completed","2019-11-04T23:59:35","No","No","No","Internal"]
[null,null,null,6245,null,"48_2019-08-11 09:43:02.000","2019-10-27T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Water cooler in officer mess room was kept in isolated condition due to leak. TO be made operational.","Accommodation","MLC Related","Equipment Related","11.13","Low","","","Fountain tap leak was rectified. System back in operation. ","2019-11-10T23:59:35","","Completed","2019-11-05T23:59:35","No","No","No","Internal"]
[null,null,null,6246,null,"48_2019-11-08 19:44:49.998","2019-10-27T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Both boiler gauge glass light not working.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Light changed. ","2019-11-06T23:59:35","","Completed","2019-11-06T23:59:35","No","No","No","Internal"]
[null,null,null,6248,null,"48_43688.8260185185","2019-10-27T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","MSDS and PPE to place in BWTS room for neutralizing chemicals.","Cargo Mach.","Cargo / Ballast Systems","Inappropriate Procedure","10.32","Very High","","","MSDS Put in place in BWTS room for Neutralizer chemicals, Sodium hypochlorite & hydrogen gas.","2019-11-06T23:59:35","","Completed","2019-11-01T23:59:35","No","No","No","External"]
[null,null,null,8611,null,"48_Fri Nov 08 2019 20:13:51 GMT+0000 (Coordinated Universal Time)","2019-10-27T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ME LO auto filter shaft seal leaking. To be renewed","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Will be renewed in the first oppurtunity. L.O. BACKWASH FILTER SERVICE CARRIED OUT. ALL CANDLES REPLACED WITH CLEANED SPARE. TOP X-OIL SEAL(2PCS) REPLACED WITH NEW SPARE.","2019-12-11T23:59:35","","Completed","2019-12-04T23:59:35","No","No","No","External"]
[null,null,null,7090,null,"48_Sun Aug 11 2019 09:37:39 GMT+0000 (Coordinated Universal Time)","2019-10-27T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Mooring wires are covered with mud due to use in yard. Cleaning and greasing required.","Miscellaneous","Mooring","Equipment Related,External Factors","9.17","High","","","Mud cleaning & Greasing of all the 10 mooring wires in fwd carried out. Remaining all 10 ropes in the aft station were thorougly washed of the mud - Greasing was found in good condition on them. Both the fire wires greasing also done.","2020-01-27T23:59:35","","Completed","2019-12-11T23:59:35","No","No","No","Internal"]
[null,null,null,7094,null,"48_Sun Aug 11 2019 10:25:48 GMT+0000 (Coordinated Universal Time)","2019-10-27T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","All the PV valves inspection date stencil to change.","Deck - Pipe / Fittings","General Appearance","Equipment Related","8.21","High","","","Overhauling dates stencilling done on all PV valve.","2019-11-21T23:59:35","","Completed","2019-11-02T23:59:35","No","No","No","Internal"]
[null,null,null,7095,null,"48_Sun Aug 11 2019 10:29:34 GMT+0000 (Coordinated Universal Time)","2019-10-27T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Outside pump room Stbd side air valve leaking, To be renewed.","Deck - Pipe / Fittings","Eng. / Strg. Comp.","Equipment Related","11.4","Very High","","","air manifold valve renewed.","2019-11-11T23:59:35","","Completed","2019-11-09T23:59:35","No","No","No","Internal"]
[null,null,null,7096,null,"48_Sun Aug 11 2019 19:49:28 GMT+0000 (Coordinated Universal Time)","2019-10-27T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","MSDS and PPE to place in BWTS room for neutralizing chemicals.","Cargo Mach.","Cargo / Ballast Systems","Inappropriate Procedure","10.32","Very High","","","MSDS AND PPE put in place in BWTS room","2019-11-06T23:59:35","","Completed","2019-11-01T23:59:35","No","No","No","External"]
[null,null,null,7097,null,"48_Sun Aug 11 2019 10:45:11 GMT+0000 (Coordinated Universal Time)","2019-10-27T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Fire line pipe in scrubber room, just above the main power panel vibrates a lot at higher RPM. More supports to be welded. ","LSA / FFA","Eng. / Strg. Comp.","External Factors","11.5","Medium","","","fitted extra supports on the pipeline.","2019-11-11T23:59:35","","Completed","2019-11-11T23:59:35","No","No","No","Internal"]
[null,null,null,7098,null,"48_Fri Nov 08 2019 20:02:45 GMT+0000 (Coordinated Universal Time)","2019-10-27T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Zebra stripe sticker to put in the newly installed low head pipe in  ER bottom platform","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","External Factors","10.32","Very High","","","Out the stripes stickers. ","2019-11-03T23:59:35","","Completed","2019-11-08T23:59:35","No","No","No","External"]
[null,null,null,7099,null,"48_Fri Nov 08 2019 19:51:48 GMT+0000 (Coordinated Universal Time)","2019-10-27T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Various electrical insulation mat in E/R and emergency DG room are deteriorated or salt soaked. To be renewed.","Miscellaneous","Eng. / Strg. Comp.","Inappropriate Procedure","11.11","Very High","","","REPLACED THE INSULATION MATS","2019-11-05T23:59:35","","Completed","2019-11-20T23:59:35","No","No","No","External"]
[null,null,null,6247,null,"48_16/11/2019 8:59:18 AM","2019-11-05T23:59:35","Guarantee Claim","Ship Staff","Ship Staff Insp.","BWTS filter inlet valves BT-1211 & BT-2211 not operating in remote or Local mode. No power available on the valve actuator display unit because of faulty PCB in the valve actuators.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.14","Very High","","","PCBs renewed and close/Open calibration carried out also new PCB renewed setting done . now valve can be operated from local and remote as well","2020-02-05T23:59:35","","Completed","2020-02-02T23:59:35","No","No","No","Internal","GC spares have been received, will be supplied at next convenient port."]
[null,null,null,6149,null,"48_25/10/2019 3:17:08 PM","2019-11-09T23:59:35","Defect","Ship Staff","Ship Staff Insp.","APK WBT gauge showing erratic reading","Elect. Mach. & Equip.","Cargo / Ballast Systems","Equipment Related","8.12","Medium","","","New level sensor received and fitted. APK WBT guage calibrated and working satisfactory.","2020-02-09T23:59:35","STAI190182","Completed","2020-02-02T23:59:35","No","No","No","Internal","Target date revised as the spares are not yet ready. Please mention correct RO no."]
[null,null,null,8605,null,"48_Mon Dec 09 2019 23:52:54 GMT+0000 (Coordinated Universal Time)","2019-11-10T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Others (Eg. Insurance etc.)","CCR Movement Book - No entry for Line draining sighted after completion of Loading on 18 July 2019 and completion of discharging on 10th Sept 2019. ","Documentation","Cargo / Ballast Systems","Human Error","8.5","Very High","","","Noted, Line draining missed out for writing in the CCR log but please note that Line draining is part of the ''12.80.13.094.00 Completion of cargo & Pre departure checklist'' checklist and it has been filed there. Copy attached.\n\nPreventive action : Discussed with all officers & will ensure line draining enteries and timings to be maintained in CCR log as well.  \n\n","2019-11-21T23:59:35","","Completed","2019-11-21T23:59:35","No","No","No","Internal"]
[null,null,null,8606,null,"48_Thu Sep 12 2019 23:55:21 GMT+0000 (Coordinated Universal Time)","2019-11-10T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Others (Eg. Insurance etc.)","Ship Shore Safety Checklist dated 17 July 2019 Pt 33 - No comment entered in Remarks.","Documentation","Cargo / Ballast Systems","Human Error","5.9","Very High","","","Comment added in point 33. All recent checklists verified that all items are completed properly.Discussed with all officers & will ensure all relevent A items are marked with comments\n\n","2019-11-21T23:59:35","","Completed","2019-11-21T23:59:35","No","No","No","Internal"]
[null,null,null,8607,null,"48_Thu Sep 12 2019 23:57:23 GMT+0000 (Coordinated Universal Time)","2019-11-10T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Others (Eg. Insurance etc.)","No entry for Operational Test of Cargo and ballast hydraulic valves sighted prior Load Port GOLA,US","Documentation","Cargo / Ballast Systems","Behaviour Based,Human Error","8.5","Very High","","","Operational test of cargo and ballast hydraulic valves already written under ''Cargo valves hydraulic system tried out, hydraulic tank level checked'' on page 90 of CCR log. Copy attached & highlighted.\n\nPreventive action : Discussed with all officers & will ensure that all individual valves for ballast & cargo system to be tried out and entry in the CCR log to be written clearly.\n\n","2019-11-21T23:59:35","","Completed","2019-11-21T23:59:35","No","No","No","Internal"]
[null,null,null,8608,null,"48_Tue Dec 10 2019 00:00:24 GMT+0000 (Coordinated Universal Time)","2019-11-10T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Bunkering Audit","Bunker Transfer Plan / Checklist 12.04.08.011.01 Section 7 - Monitoring of H2S/Benzene Vapors : \n\nBenzene reading measured by detector tubes shall be mentioned < Min value that can be measured by the specific tube. For example by Gastec tubes Min measurable value is 0.05 ppm, hence in that case benzene shall be mention <0.05 ppm (if no discoloration observed)\n\nUnderstand vessel has kept the Gas tubes as evidence of monitoring.\n\n","Documentation","Eng. / Strg. Comp.","Human Error","5.9","Very High","","","As per checklist, the Primary System :UHF Ch-2 and Secondary System :VHF Ch-16 and same updated for backup communication system. Copy attached. \n\nDiscussed with all engineer's regarding specifying the communication system established with bunker barge in the checklist properly. \n\n","2019-11-21T23:59:35","","Completed","2019-11-21T23:59:35","No","No","No","Internal"]
[null,null,null,8609,null,"48_Sat Oct 12 2019 00:02:53 GMT+0000 (Coordinated Universal Time)","2019-11-10T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Bunkering Audit","Bunker Safety Checklist for FO dated 06 Nov 2019 - Backup communication system not agreed and remarked in Pt 7 of the checklist. ","Documentation","Eng. / Strg. Comp.","Human Error","5.9","Very High","","","As per checklist, the Primary System :UHF Ch-2 and Secondary System :VHF Ch-16 and same updated for backup communication system. Copy attached. \n\nDiscussed with all engineer's regarding specifying the communication system established with bunker barge in the checklist properly. \n\n","2019-11-21T23:59:35","","Completed","2019-11-21T23:59:35","No","No","No","Internal"]
[null,null,null,6146,null,"48_25/10/2019 2:53:02 PM","2019-11-12T23:59:35","Critical Equipment","Ship Staff","Ship Staff Insp.","Display for OWS Bilge Mon not clear when seen from front, however can be seen at certain angle","Critical Equip.","Eng. / Strg. Comp.","Equipment Related","10.37","Medium","","","Display unit Brightness/contrast settings adjusted as per mail from makers. LCD display clear and bright. ","2020-02-12T23:59:35","STAI190136","Completed","2020-05-20T23:59:35","No","No","No","Internal","Maker analysis with the new display is still awaited. Target date revised."]
[null,null,null,8604,null,"48_Thu Sep 12 2019 23:35:23 GMT+0000 (Coordinated Universal Time)","2019-11-15T23:59:35","Defect","Ship Staff","Nav Audit / Verification","When Gyro compass error is not taken during a watch due to bad weather overast skies , this matter is not entered in the Compass error book.","Documentation","Navigation","Behaviour Based,Human Error","4.9","Medium","","","All duty officers were briefed that there should be atleast 6 entries in the compass error book every day when the vessel is at sea. And Duty officers have started entering the reason for not obtaining compass error evry watch.","2019-11-21T23:59:35","","Completed","2019-11-15T23:59:35","No","No","No","Internal"]
[null,null,null,7092,null,"48_Sun May 12 2019 14:13:21 GMT+0000 (Coordinated Universal Time)","2019-11-16T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Mechanical seal leaking for NO.2 Econimiser feed pump","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","To change the seal. SUPDT. COMMENT NOTED. VSL HAS SPARE SEAL. PLANNED FOR 3rd WEEK DECEMBER DUE TO BUSY SCHEDULE AT BONNY LOAD PORT. Economiser Feed water Pump No 2 overhauled as the mechanical seal was leaking. Pump was found in seized condition as part of mechanical seal carbon was found stuck in the casing. Pump opened up. Impellers were cleaned. Gaskets were changed. New mechanical seal was put along with new bearings. \n\nPump tried out and all found satisfactory.","2019-12-22T23:59:35","","Completed","2019-12-21T23:59:35","No","No","No","Internal","Target date revised due to load port. TO be completed after load port"]
[null,null,null,9497,null,"48_10/01/2020 6:12:13 AM","2019-12-21T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","BWTS valve BT2213 inside pumproom - valve motor connected with hydraulic oil cylinder got dislodged from actuator which was assembled with four bolts, These bolts may have come loose due to high vibration in pumproom. The gauge glass on hydraulic tank observed assembled in horizontal direction which makes it difficult for staff to gauge the level of oil inisde cylinder.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","Motor fixed back to actuator. Gauge glass turned in vertical position by turning the cylinder. Lost hydraulic oil replenished. Purging of hydraulic lines carried out. Valve calibration carried out. Valve tested and found operating satisfactory from remote control and local control. Cleaning of area around the valve carried out.","2019-12-27T23:59:35","","Completed","2019-12-25T23:59:35","No","No","No","Internal"]
[null,null,null,9496,null,"48_10/1/2020 10:17:47 AM","2019-12-25T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Tube light fittings all around Vsl converted wrongly to LED fittment, without disconnecting choke/ ballast, capacitor.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","11.1","High","","","Changed all tubelights to LED along with wiring.","2020-12-22T23:59:35","","Completed","2020-12-08T23:59:35","No","No","No","Internal","When is it supposed to be completed?"]
[null,null,null,9926,null,"48_20/1/2020 5:57:04 PM","2020-01-10T23:59:35","Guarantee Claim","Ship Staff","Ship Staff Insp.","Sea water temperature sensor faulty. (TE-1111) ","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.12","Medium","","","Sensor renewed with new spare received under GC. Temperature sensor working in order.","2020-02-19T23:59:35","BWTS GC - 001/2020","Completed","2020-02-25T23:59:35","No","No","No","Internal"]
[null,null,null,9927,null,"48_20/1/2020 6:04:25 PM","2020-01-10T23:59:35","Guarantee Claim","Ship Staff","Ship Staff Insp.","BWTS filter inlet valves BT-2211 not closing from local control. Suspect the switch in the local faulty or some function of PCB not responding","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.14","Very High","","","After changing the PCB,Close and Open calibration carried out and new PCB change settings done, now the valve is working from remote and local as well","2020-02-19T23:59:35","","Completed","2020-02-03T23:59:35","No","No","No","Internal"]
[null,null,null,10174,null,"48_27/01/2020 7:20:58 PM","2020-01-11T23:59:35","Defect","Ship Staff","Ship Staff Insp.","The air pressure regulator valve for ME Autobackwash filter faulty","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","As there was lack of spare, the air pressure regulator from Gas detection system was used. Job was completed and now its working fine","2020-01-12T23:59:35","","Completed","2020-01-11T23:59:35","No","No","No","Internal"]
[null,null,null,10523,null,"48_03/02/2020 19:21:47","2020-01-16T23:59:35","Defect","Ship Staff","Ship Staff Insp.","2P HFO bunker tnak Heating coil steam return line leaking from flange gasket after the return valve","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Flange gasket to be renewed after closing the main steam valve .","2020-01-23T23:59:35","","Completed","2020-01-23T23:59:35","No","No","No","Internal"]
[null,null,null,10524,null,"48_10/02/2020 7:12:35 PM","2020-01-18T23:59:35","Defect","Ship Staff","Ship Staff Insp.","FPK TANK VENT – During routine inspection of WBT vent heads, observed Float plate top tube type fitting missing (2 Nos. - Port & stbd side vent heads) from float due to which the floats were lying tilted on the support stud and eventually vent lost functionality.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","11.7","High","","","Float guide tube fabricated in e/room workshop for both the floats and welded on the floats. Both the floats fixed back on the vent heads. The support nut inside the vent head have fixed height, so height cannot be adjusted. Both the floats after repair tested for proper functioning and found operating satisfactory.","2020-01-27T23:59:35","","Completed","2020-01-25T23:59:35","No","No","No","Internal"]
[null,null,null,10512,null,"48_10/02/2020 7:37:42 PM","2020-01-23T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Paint failure noticed at few places on deck","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.3","Medium","",""," Paint failure near aft and forward  mooring winches attended. Job completed.","2020-03-23T23:59:35","","Completed","2020-03-23T23:59:35","No","No","No","Internal"]
[null,null,null,10513,null,"48_8/2/2020 10:54:45 AM","2020-01-23T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Ship Staff Insp.","Galley drain pipe stbd side has soft patch to repair","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","External Factors","10.31","Very High","","","Pipe removed and hotwork carried out in ER workshop. Pipe fitted back and No leaks from the line. Working in order.","2020-02-20T23:59:35","","Completed","2020-02-08T23:59:35","No","No","No","Internal"]
[null,null,null,10514,null,"48_8/2/2020 10:57:56 AM","2020-01-23T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","HP drum feed water valve leaking from gland, to repair","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","New valve received renewed and no leaks from the valve.","2020-03-06T23:59:35","","Completed","2020-03-20T23:59:35","No","No","No","Internal","What is RO no of the ordered valve?"]
[null,null,null,10515,null,"48_15/02/2020 12:16:29 AM","2020-01-23T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Workshop entrance door is in bent condition. To repair or to order new. Door of spare part room has its lock knob broken. To renew","Miscellaneous","Eng. / Strg. Comp.","External Factors","","","","","New door received at Singapore on 04 June 2020 and replaced .","2020-04-20T23:59:35","STAI200063","Completed","2020-05-27T23:59:35","No","No","No","Internal","Doors are ready in Singapore and will be supplied at next call Singapore."]
[null,null,null,10516,null,"48_15/02/2020 12:21:41 AM","2020-01-23T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Various markings from yard is still not painted off in engine room","Miscellaneous","Eng. / Strg. Comp.","External Factors","","","","","Markings are painted off/wiped clean.","2020-03-22T23:59:35","","Completed","2020-03-16T23:59:35","No","No","No","Internal"]
[null,null,null,10517,null,"48_15/02/2020 12:26:36 AM","2020-01-23T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Cracked light cover in pump room to renew","Elect. Mach. & Equip.","Cargo / Ballast Systems","Equipment Related","11.11","Very High","","","all cracked light fittings renewed with LED conversion.","2020-03-06T23:59:35","","Completed","2020-03-14T23:59:35","No","No","No","Internal"]
[null,null,null,10518,null,"48_15/02/2020 12:30:50 AM","2020-01-23T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","All engine room blower mushroom vent to de-rust and paint\t","E/R - Aux. Mach.","General Appearance","Equipment Related","","","","","e/r blower derusting and full coat painting completed","2020-03-22T23:59:35","","Completed","2020-03-11T23:59:35","No","No","No","Internal"]
[null,null,null,10519,null,"48_15/02/2020 12:34:07 AM","2020-01-23T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Both lifeboat motor and related area to derust and paint","Hull & Tanks","General Appearance","External Factors","5.29","High","","","Derusted and painted areas near lifeboat motor oil tank and related areas.Reported to office in weekly workdone report with photos","2020-02-11T23:59:35","","Completed","2020-02-11T23:59:35","No","No","No","Internal"]
[null,null,null,10520,null,"48_15/02/2020 12:37:06 AM","2020-01-23T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Removed spare VCU and fuel pump to overhaul","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Spare VCU overhauled and ME fuel pump overhauled with new plunger barell and o-rings. Both marked and kept as standby ","2020-02-20T23:59:35","","Completed","2020-03-04T23:59:35","No","No","No","Internal"]
[null,null,null,10521,null,"48_15/02/2020 12:39:02 AM","2020-01-23T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","EGB casing and area cleaning\t","Miscellaneous","General Appearance","External Factors","10.29","Medium","","","Cosmetic upgradation Completed . Area cleaned and painted after receiving the paints.","2020-02-21T23:59:35","","Completed","2020-04-04T23:59:35","No","No","No","Internal","It is long pending job, when it expected to complete."]
[null,null,null,10522,null,"48_15/02/2020 12:42:53 AM","2020-01-23T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Aft deck below scrubber house needs to hydroblast and paint\t","Hull & Tanks","General Appearance","External Factors","11.3","Medium","","","Hydroblasted and full area beneath EGS unit painted with antiskid surface.","2020-03-11T23:59:35","","Completed","2020-03-05T23:59:35","No","No","No","Internal"]
[null,null,null,10525,null,"48_8/2/2020 11:00:47 AM","2020-01-23T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Emergency DG room fuel filter leaking, oil collected below it. To rectify\t\t","Critical Equip.","Emgcy. Systems","Equipment Related","10.35","Very High","","","Filter drain tightened and leak rectified","2020-01-27T23:59:35","","Completed","2020-01-26T23:59:35","No","No","No","Internal"]
[null,null,null,10526,null,"48_8/2/2020 11:03:10 AM","2020-01-23T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","In EGCS room slight SW leak from one of the flange. \t","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Tightened bolts of flanges. ","2020-02-01T23:59:35","","Completed","2020-01-27T23:59:35","No","No","No","Internal"]
[null,null,null,10527,null,"48_15/02/2020 12:32:36 AM","2020-01-23T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Boiler safety valve flange not covered with lagging\t","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","New lagging fabricated and flanges covered up","2020-01-29T23:59:35","","Completed","2020-01-27T23:59:35","No","No","No","Internal"]
[null,null,null,10528,null,"48_15/02/2020 12:19:29 AM","2020-01-23T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Sewage treatment plant chlorine pump in running condition but there is no flow of liquid. Flow indicator dirty and float is not visible\t","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Chlorine pump primed and operation checked and verified. Flow indicator cleaned. Sewage plant working in order","2020-02-01T23:59:35","","Completed","2020-01-25T23:59:35","No","No","No","Internal"]
[null,null,null,10529,null,"48_15/02/2020 12:41:19 AM","2020-01-23T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Save all of bilge tank, hot well to clean. Vent heads needs cleaning","Hull & Tanks","General Appearance","Inappropriate Procedure","11.7","High","","","Save all cleaned and painted. All vents heads inspected, cleaned and painted.","2020-01-26T23:59:35","","Completed","2020-01-26T23:59:35","No","No","No","Internal"]
[null,null,null,10530,null,"48_15/02/2020 12:44:33 AM","2020-01-23T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Steering gear room aft bilges to mark yellow\t","Miscellaneous","Eng. / Strg. Comp.","Inappropriate Procedure","10.32","Very High","","","Bilges marked yellow ","2020-01-29T23:59:35","","Completed","2020-01-26T23:59:35","No","No","No","Internal"]
[null,null,null,10531,null,"48_15/02/2020 12:28:33 AM","2020-01-23T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Foam pump has leakage marks. To be checked while running and seals to renew if required\t","LSA / FFA","Safety / LSA / FFA","Equipment Related","10.29","Medium","","","Mechanical seal renewed and pump tried out no leaks","2020-02-01T23:59:35","","Completed","2020-02-06T23:59:35","No","No","No","Internal"]
[null,null,null,10532,null,"48_15/02/2020 12:23:49 AM","2020-01-23T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Steam ballast pump to overhaul as same is leaking from seal\t","Deck - Machinery","Eng. / Strg. Comp.","Equipment Related","10.31","Very High","","","Mechanical seal of ballast pump renewed , pump tried out no leaks","2020-02-06T23:59:35","","Completed","2020-02-06T23:59:35","No","No","No","Internal"]
[null,null,null,10743,null,"48_3/3/2020 6:16:25 PM","2020-02-06T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Drain line from IGS scrubber tower found to have hole and water leaking\t\t","Inert Gas","Eng. / Strg. Comp.","Equipment Related","8.22","Very High","","","Hot work carried out after permission from office. Drain pipe with flange fabricated and welded. ","2020-02-16T23:59:35","","Completed","2020-02-09T23:59:35","No","No","No","Internal"]
[null,null,null,10749,null,"48_4/3/2020 10:39:17 AM","2020-02-06T23:59:35","Defect","Ship Staff","Ship Staff Insp.","IGS scrubber tower drain pipe leak to rectify.","Inert Gas","Eng. / Strg. Comp.","Equipment Related","8.22","Very High","","","Leak from drain pipe rectified with hotwork after office approval.  New pipe welded as the old pipe found to have corroded badly. New pipe after welding coated with epoxy. Scrubber system tried out no leaks observed.","2020-02-20T23:59:35","","Completed","2020-02-09T23:59:35","No","No","No","Internal"]
[null,null,null,10744,null,"48_3/3/2020 6:20:13 PM","2020-02-12T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Sewage treatment plant Air Blower #2 tripping on overload.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Sewage plant air blower #2 overhauled, found driving end bearing seized. Both end bearing renewed and tried out. Working satisfactory.","2020-02-20T23:59:35","","Completed","2020-02-13T23:59:35","No","No","No","Internal"]
[null,null,null,10750,null,"48_4/3/2020 10:45:10 AM","2020-02-12T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Sewage treatment plant no:2 air blower found to trip on overload.\t","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","No:2 air blower motor driving end bearing found to be seized. Both end bearings renewed and tried out. working in order.","2020-02-20T23:59:35","","Completed","2020-02-13T23:59:35","No","No","No","Internal"]
[null,null,null,10741,null,"48_01/03/2020 6:00:37 PM","2020-02-16T23:59:35","Breakdown,Defect","Ship Staff","Ship Staff Insp.","Two UTIs onboard has developed following errors: -\tUTI # G17710: LED display stopped working. Unable to see temperature readings. Last shore calibration of UTI: 07-Jan-2020. - UTI # 66433 : Temperature readings showing difference of more than 3 deg C and sometimes even more than other UTIs & thermometer. Last shore calibration of UTI: 05-Oct-2019.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.12","Medium","","","Two new UTIs with shore calibration received on 04-Mar-2020 at Singapore EOPL. UTI #17927 & 17928 (Shore calibration date: 27-Feb-2020). Both UTIs tested and found suitable for vessel use.","2020-03-01T23:59:35","STAI205021","Completed","2020-02-24T23:59:35","No","No","No","Internal","already supplied passing Singapore."]
[null,null,null,10747,null,"48_04/03/2020 21:12:33","2020-02-16T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","Two UTIs onboardhas devolopedfollowing errors:UTI#G17710:LED display stopped working.Unable to see temperature readings.Last shore calibration of UTI07 Jan 2020-UTI #66433","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.12","Medium","","","Two new UTIs with shore calibration received on 04-Mar-2020 at Singapore EOPL. UTI #17927 & 17928 (Shore calibration date: 27-Feb-2020). Both UTIs tested and found suitable for vessel use.","2020-03-01T23:59:35","STAI205021","Completed","2020-02-24T23:59:35","No","No","No","Internal"]
[null,null,null,10742,null,"48_03/03/2020 3:11:00 PM","2020-02-19T23:59:35","Defect","Ship Staff","Ship Staff Insp.","4P & 5S WBT Level gauges faulty","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.12","Medium","","","Same defect was duplicated. ","2020-04-22T23:59:35","STAI200080","Completed","2020-02-19T23:59:35","No","No","No","Internal","Awaiting  readiness of spares."]
[null,null,null,10837,null,"48_15/03/2020 3:40:49 PM","2020-02-27T23:59:35","Defect","Ship Staff","Ship Staff Insp.","HP drum PORT water level guage glass  leaking","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","HP drum water level guage glass overhauled. New glass and gaskets changed. No leaks observed","2020-03-06T23:59:35","","Completed","2020-02-28T23:59:35","No","No","No","Internal"]
[null,null,null,10836,null,"48_15/03/2020 3:44:08 PM","2020-03-02T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Inert gas Generator system gas outlet digital temperature indicator faulty","Inert Gas","Eng. / Strg. Comp.","Equipment Related","8.22","Very High","","","New Spare digital indicator received atSingapore on 04 June 2020 and replaced now working ok.","2020-06-02T23:59:35","STAI200082","Completed","2020-05-27T23:59:35","No","No","No","Internal","Awaiting readiness."]
[null,null,null,11454,null,"48_31/3/2020 11:56:39 PM","2020-03-11T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Main Engine Waste gate for exhaust manifold solenoid valve not operational.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","New spare solenoid valve received at Singapore on 04 june 2020 and defective one replaced with new spare . now working ok.","2020-06-21T23:59:35","STAI200075","Completed","2020-06-04T23:59:35","No","No","No","Internal","Will be ready by 5th June 20"]
[null,null,null,7093,null,"48_Sun May 12 2019 14:15:56 GMT+0000 (Coordinated Universal Time)","2020-03-17T23:59:35","Defect","Ship Staff","Ship Staff Insp.","The slewing limit valve for STBD provision crane is defective and broken.","Deck - Machinery","Eng. / Strg. Comp.","External Factors","8.5","Very High","","","change the spare limit switch. tried out.","2020-09-21T23:59:35","STAI200148","Completed","2020-09-29T23:59:35","No","No","No","Internal","Order RO for limit valve as these has long lead time. Target date revised."]
[null,null,null,11453,null,"48_9/4/2020 7:57:07 AM","2020-03-17T23:59:35","Defect","Ship Staff","Ship Staff Insp.","ECR AC #1 fan abnormal noise & vibrations","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","New blower received at singapore on 10th july and fitted back. Tried our working satisfactory.","2020-05-22T23:59:35","STAI200092","Completed","2020-07-04T23:59:35","No","No","No","Internal"]
[null,null,null,11455,null,"48_31/3/2020 11:51:13 PM","2020-03-20T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Spare parts inventory to update in PAL\t","Miscellaneous","Eng. / Strg. Comp.","Knowledge Based","","","","","\n\n\n\nSpare part inventory updated","2020-06-21T23:59:35","","Completed","2020-06-19T23:59:35","No","No","No","Internal"]
[null,null,null,11456,null,"48_17/4/2020 5:01:47 AM","2020-04-03T23:59:35","Defect","Ship Staff","Ship Staff Insp.","No.2 Ejector pump for FWG Mech. seal found leaking and pump found to be fitted in reverse direction . Suction /Discharge orientation wrong in last dry dock","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.31","Very High","","","Pump overhauled and mech seal renewed ,all clearances taken . Pump installed in right direction and suction /Discharge pipe modification  carried out. Pump tried out and FWG running satisfactory.","2020-04-11T23:59:35","","Completed","2020-04-06T23:59:35","No","No","No","Internal"]
[null,null,null,9928,null,"48_20/1/2020 6:07:05 PM","2020-04-10T23:59:35","Guarantee Claim","Ship Staff","Ship Staff Insp.","APK Tank Level Sensor (AP-LVL-01) Faulty","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.12","Medium","","","Isolation converter received and installed in the circuit , Aft peak level found working ok in both Tank Radar and BWTS without any issue. No spares required, level sensor working satisfactory.","2021-01-21T23:59:35","","Completed","2021-01-19T23:59:35","No","No","No","Internal","Awaiting maker advise. Target date revised"]
[null,null,null,11520,null,"48_01/05/2020 3:45:16 AM","2020-04-11T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Steam Leak from condensate return pipe at ER 3rd Deck to be rectified.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Steam leaks rectified, flange gaskets renewed.","2020-04-29T23:59:35","","Completed","2020-04-24T23:59:35","No","No","No","Internal"]
[null,null,null,11521,null,"48_01/05/2020 3:49:19 AM","2020-04-13T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Steering gear room vacuum toilet unit not working\t","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","vacuum toilet unit overhauled missing parts replaced with new spare. tried out working satisfactory Spare received @ Singapore on 10th July 2020.","2020-05-22T23:59:35","STAI200110","Completed","2020-07-07T23:59:35","No","No","No","Internal"]
[null,null,null,11844,null,"48_14/05/2020 3:38:38 AM","2020-04-16T23:59:35","Critical Equipment","Ship Staff","Ship Staff Insp.","MF/HF unit is not transmitting DSC Test Alerts with coast stations and other ships","Navigation - GMDSS & Communication","Communication","Equipment Related","4.24","High","","","Complete MF/HF Unit replaced with Upgraded one ( Latest Version)  at Singapore on 11 July 2020.","2020-06-03T23:59:35","","Completed","2020-07-02T23:59:35","No","No","No","Internal","Service being arranged in Tianjin."]
[null,null,null,11845,null,"48_14/05/2020 3:46:15 AM","2020-04-16T23:59:35","Critical Equipment","Ship Staff","Ship Staff Insp.","Aft transducer unit is not relaying signals to echosunder display unit on bridge","Navigation - Echo Sounder / Speed Log","Navigation","Equipment Related","4.7","High","","","Aft transducer sensor with cable renewed at Singapore on 11 July 2020. now working ok ","2020-06-03T23:59:35","","Completed","2020-07-02T23:59:35","No","No","No","Internal"]
[null,null,null,13183,null,"48_05/07/2020 10:51:05 AM","2020-05-03T23:59:35","Defect","Ship Staff","Ship Staff Insp.","FPK TANK VENT – During routine inspection of WBT vent heads, observed Float plate top tube type fitting missing (2 Nos. - Port & stbd side vent heads) from float due to which the floats were lying tilted on the support stud and eventually vent lost functionality.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","11.7","High","","","FP WBT float replaced 2nos with new floats received onboard at Singapore. FPT vesnt in good working condition ","2020-08-22T23:59:35","STAI200124","Completed","2020-08-02T23:59:35","No","No","No","Internal","Correct size vent already supplied. Fit ASAP."]
[null,null,null,12018,null,"48_19/05/2020 20:02:49","2020-05-10T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Port life boat Alarm and Indicating Buzzer defective and not Operational.","LSA / FFA","Emgcy. Systems","Equipment Related","5.29","High","","","New spare Buzzer received at Singapore on 04 June 2020 , defective buzzer replaced with new spare received and now working ok","2020-05-27T23:59:35","STAI200122","Completed","2020-05-27T23:59:35","No","No","No","Internal"]
[null,null,null,10748,null,"48_04/03/2020 21:17:43","2020-05-17T23:59:35","Defect","Ship Staff","Ship Staff Insp.","4P & 5S WBT Tank radar remote level gauges Faulty","Hull & Tanks","Cargo / Ballast Systems","Equipment Related","8.12","Medium","","","Spares reveived & 4P, 5S WBT sensors replaced with new sensor supplied at Singapore on 15 Oct 2020. System working satisfactorily","2021-01-21T23:59:35","STAI200080","Completed","2020-10-07T23:59:35","No","No","No","Internal","New spares will be supplied at next opportunity. Target date revised due to readiness of spares."]
[null,null,null,12999,null,"48_03/07/2020 21:00:45","2020-06-13T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Aft hydraulic mooring winch oil return pipe leaking as pipe found corroded and wasted ","Deck - Mooring Machinery","Mooring","Equipment Related","9.14","Medium","","","After departure pipe removed and new pipe fabricated and fitted back , tried out found ok","2020-06-16T23:59:35","","Completed","2020-06-15T23:59:35","No","No","No","Internal"]
[null,null,null,13184,null,"48_05/07/2020 12:24:02 PM","2020-06-22T23:59:35","Defect","Ship Staff","Ship Staff Insp.","During recent discharging operations at Qingdao and Tianjin, following centre tanks COW machines found not working during \n\n\n\n1C- Nos. 1, 2 & 4 / 2C - nos. 1, 2, & 4 / 3C- No.4 / 4C - No.3 / 5C - Nos. 1, 2, 3 & 4. Oil was passing through these machines but they were not rotating. Follow up on status of COW machines carried out during discharging at Ningbo, China.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.34","High","","","Complete overhaul of COW machines carried out. 1C: TC10, 2C: TC22, 5C: TC53.\n\nMachines tested by turning with allen key, found in good working condition.\n\nLower magnet found damaged due to scratch marks, same replaced. \n\n","2020-08-23T23:59:35","","Completed","2020-08-30T23:59:35","No","No","No","Internal","Understand all COW machine except 3 are ok and overhauling of 3 are in progress. target date revised accordingly."]
[null,null,null,13194,null,"48_16/7/2020 12:25:00 PM","2020-06-24T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Port waste water pipe before storm valve found pinhole on on side near storm valve.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Pipe dismantled and repaired. Painted with epoxy primer paint and fitted back in place. Tested found no leak.","2020-07-02T23:59:35","","Completed","2020-07-02T23:59:35","No","No","No","Internal"]
[null,null,null,13195,null,"48_16/7/2020 12:39:23 PM","2020-06-26T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Waste water overboard valve gasket leaking on the outboard side of storm valve.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Gasket replaced with new one after divers plugged the line. tested no leak.","2020-07-02T23:59:35","","Completed","2020-07-02T23:59:35","No","No","No","Internal"]
[null,null,null,13196,null,"48_16/7/2020 12:47:09 PM","2020-06-27T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Port waste water overboard valve found not holding, suspected storm valve damaged","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Valve replaced with new spare after the divers plugged the line. Tested and no leak","2020-07-02T23:59:35","","Completed","2020-07-02T23:59:35","No","No","No","Internal"]
[null,null,null,13182,null,"48_17/07/2020 10:04:46 AM","2020-07-01T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Stencil the certificate no on both chain stopper and punch mark it for its permanency.","Deck - Mooring Machinery","General Appearance","Equipment Related","11.2","Medium","","","Permanent Beed welded certificate already exists on chain stoppers. Certificate number stencilled on both the chain stoppers","2020-07-22T23:59:35","","Completed","2020-07-11T23:59:35","No","No","No","Internal"]
[null,null,null,13185,null,"48_17/07/2020 9:56:16 AM","2020-07-01T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Cargo line dresser coupling bolts are rusted at various locations, to be renewed.","Deck - Pipe / Fittings","General Appearance","Equipment Related","8.3","Very High","","","Completed maintenance of dresser couplings bolts of Cargo, COW, Fire, IG line on deck","2021-01-21T23:59:35","","Completed","2021-01-04T23:59:35","No","No","No","Internal"]
[null,null,null,13186,null,"48_17/07/2020 9:58:55 AM","2020-07-01T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Insulation sleeve of Sound receptacle in fore peak store is damaged. Sleeve to renew.","Navigation - GMDSS & Communication","General Appearance","Equipment Related","","","","","Sleeve renewed.","2020-07-20T23:59:35","","Completed","2020-07-12T23:59:35","No","No","No","Internal"]
[null,null,null,13187,null,"48_17/07/2020 10:00:36 AM","2020-07-01T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Provision cranes boom derusting and painting to be carried out.","Deck - Machinery","General Appearance","Equipment Related","11.1","High","","","Derusting & full coat painting of P & S Provision crane completed.","2020-08-16T23:59:35","","Completed","2020-08-25T23:59:35","No","No","No","Internal","Target date revised as requested."]
[null,null,null,13188,null,"48_16/7/2020 12:59:46 PM","2020-07-05T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Many of the number keys of emergency DG room phone is missing","Miscellaneous","Safety / LSA / FFA","Equipment Related","11.1","High","","","Phone numbers keys replaced with new spare.","2020-08-22T23:59:35","STAI200102","Completed","2020-08-18T23:59:35","No","No","No","Internal","Spares will be supplied at next opportunity. Target date revised."]
[null,null,null,13189,null,"48_16/7/2020 1:05:07 PM","2020-07-05T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ME Cylinder heads needs to clean. There are various dry oil marks and dried salt marks present on almost all cylinder heads.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Main engine all Cylinder covers buffed and cleaned ..","2020-08-21T23:59:35","","Completed","2020-07-12T23:59:35","No","No","No","Internal"]
[null,null,null,13190,null,"48_16/7/2020 1:17:08 PM","2020-07-05T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","There is no coupling pad in spider coupling fitted between the propeller shaft and lifeboat engine","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","Coupling pad fabricated and fitted tried out found working ok.","2020-08-21T23:59:35","","Completed","2020-07-10T23:59:35","No","No","No","Internal"]
[null,null,null,13191,null,"48_16/7/2020 1:23:44 PM","2020-07-05T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Various alarm related to ACONIS were active in AMS since June and no investigation has been carried out for same.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","11.1","High","","","All alarms attended & rectified.","2020-09-21T23:59:35","","Completed","2020-09-09T23:59:35","No","No","No","Internal","Please restart Aconis Pc once vessel is at anchorage and EGCS stopped. Target date revised."]
[null,null,null,13192,null,"48_16/7/2020 1:31:13 PM","2020-07-05T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Workshop air con was not yet operational, even though new air con blower has already been supplied.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Blower replaced with new spare recieved in singapore.","2020-09-21T23:59:35","STAI200174","Completed","2020-08-30T23:59:35","No","No","No","Internal","Replacement blower  is being arranged."]
[null,null,null,13193,null,"48_16/7/2020 1:10:47 PM","2020-07-05T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Port ECR air con blower making abnormal sound.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Port ECR air con blower renewed with new spare blower recived in Singapore.","2020-09-21T23:59:35","STAI200174","Completed","2020-08-30T23:59:35","No","No","No","Internal","Will be supplied next call Singapore."]
[null,null,null,13197,null,"48_16/7/2020 12:54:49 PM","2020-07-05T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Steering Gear room drain valve (spring loaded) in engine room found to be seized","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Valve dismantled and overhauled and make it operational.","2020-07-11T23:59:35","","Completed","2020-07-07T23:59:35","No","No","No","Internal"]
[null,null,null,13198,null,"48_16/7/2020 1:26:54 PM","2020-07-05T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Echo sounder aft transducer cable was laid externally by service engineers and hence the manhole door of void space was kept open.  ","Navigation - Echo Sounder / Speed Log","Eng. / Strg. Comp.","Inappropriate Procedure","11.6","Medium","","","The laid through the Conduit pipe and Manhole door secured .","2020-07-11T23:59:35","","Completed","2020-07-08T23:59:35","No","No","No","Internal"]
[null,null,null,13331,null,"48_01/08/2020 23:14:09","2020-07-22T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Aft peak BWTS system flow control valve FCV-3211 showing sensor failure and malfunctioning.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","11.1","High","","","Received spare PCB against GC. Changed the spare. tried out working fine.","2020-08-22T23:59:35","","Completed","2020-08-04T23:59:35","No","No","No","Internal"]
[null,null,null,13332,null,"48_01/08/2020 23:23:20","2020-07-22T23:59:35","Defect","Ship Staff","Ship Staff Insp.","IG no.2 Blower discharge valve not closing properly .suspecting valve seat ring damage or excessive carbon deposite on the valve seat /valve","Inert Gas","Eng. / Strg. Comp.","Equipment Related","8.22","Very High","","","VALVE OPENED UP, FOUND DISC WAS HALF OPENED. VALVE SEAT WAS INTACTT. ADJUSTED THE ACTUATOR POSITION. TRIED OUT WORKING FINE","2020-08-22T23:59:35","STAI200170","Completed","2020-08-01T23:59:35","No","No","No","Internal","Open the valve and  clear off soot."]
[null,null,null,13534,null,"48_18/8/2020 2:49:21 PM","2020-07-24T23:59:35","Defect","Ship Staff","Ship Staff Insp.","AUX ENGINE GIVING HIGH TEMP. FOR T/C INLET","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Turbo charger nozzle ring replaced with new spare recived in singapore. Aux DG working satisfactory.","2020-09-23T23:59:35","STAI205058","Completed","2020-08-31T23:59:35","No","No","No","Internal","Please renew the nozzle ring."]
[null,null,null,13535,null,"48_18/8/2020 2:53:24 PM","2020-07-24T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","MDO FLUSHING PUMP FOR D/G NOT BUILDING PRESSURE AND LEAKING FORM THE MECHANICAL SEAL","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","CHANGED PUMP. TRIED OUT. WOKRING SATIS","2020-12-25T23:59:35","STAI 200065","Completed","2020-10-06T23:59:35","No","No","No","Internal","Will be supplied at next convenient port."]
[null,null,null,13536,null,"48_19/8/2020 10:58:08 AM","2020-07-24T23:59:35","Defect","Ship Staff","Ship Staff Insp.","EGB drain line valve not holding","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","CHANGED VALVE.","2020-09-23T23:59:35","","Completed","2020-08-24T23:59:35","No","No","No","Internal","Mention the RO number."]
[null,null,null,13537,null,"48_20/08/2020 8:13:50 AM","2020-07-24T23:59:35","Observation","Ship Staff","Ship Staff Insp.","AFT draft gauge in CCR is not operational. Feed to SAAB system in CCR is also showing \"zero\" Reading.","Miscellaneous","Cargo / Ballast Systems","Equipment Related","8.19","High","","","PCB card for aft draft gauge replaced with old(used) card available onboard, SPAN & ZERO Calibration of FAT draft gauge sensor carried out at Ningbo anchorage & found operating in satisfactory condition. ","2020-09-21T23:59:35","","Completed","2020-08-17T23:59:35","No","No","No","Internal"]
[null,null,null,13539,null,"48_19/08/2020 4:27:15 PM","2020-07-30T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Cooling water line for Hydraulic motor power pack for forward station found leaking.","Deck - Mooring Machinery","Mooring","Equipment Related","","","","","Leaking cooling water pipe fabricated onboard & replaced with leaking cooling water pipe","2020-08-08T23:59:35","","Completed","2020-08-06T23:59:35","No","No","No","Internal"]
[null,null,null,13540,null,"48_19/08/2020 4:23:13 PM","2020-08-03T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Hydraulic oil observed leaking from mooring winch M4  return line.","Deck - Mooring Machinery","Mooring","Equipment Related","11.4","Very High","","","Leaking hydraulic oil pipe fabricated onboard & installed.","2020-08-08T23:59:35","","Completed","2020-08-08T23:59:35","No","No","No","Internal"]
[null,null,null,13538,null,"48_19/08/2020 6:24:33 PM","2020-08-09T23:59:35","Defect","Ship Staff","Ship Staff Insp.","ODME Sampling pump inlet side coupling found leaking during quarterly testing of ODME. Gasket, Check valve & guide found badly damaged ","Miscellaneous","Cargo / Ballast Systems","Equipment Related","6.13","Low","","","Spares received at Singapore on 15 Oct 2020 & replaced. No leakage observed in the flange.","2021-01-11T23:59:35","STAI200197","Completed","2020-10-08T23:59:35","No","No","No","Internal"]
[null,null,null,13878,null,"48_31/08/2020 3:18:41 PM","2020-08-15T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Entrance hatch coaming of WBT 1P, 1S, 2S, 4P, 4S rusted & requires maintenance","Hull & Tanks","General Appearance","External Factors","8.59","High","","","Derusting & painting of WBT entrance hatch carried out of all WBT's. Pictures sent in weekly work done report.","2020-11-14T23:59:35","","Completed","2020-10-01T23:59:35","No","No","No","Internal"]
[null,null,null,13879,null,"48_30/08/2020 10:40:09 AM","2020-08-17T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Bridge front window No.3 wiper not operational due to broken Belt","Elect. Mach. & Equip.","Navigation","Equipment Related","12.1","High","","","Belt for window wiper motor renewed with new spare received on 6 Sep 2020 at Singapore","2020-10-22T23:59:35","STAI200176","Completed","2020-09-05T23:59:35","No","No","No","Internal","already supplied."]
[null,null,null,13880,null,"48_29/8/2020 9:57:38 AM","2020-08-20T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Galley Baking Oven Low insulation 440 volts From heating coils.","Accommodation","General Appearance","Equipment Related","11.1","High","","","Heating coils replaced.","2020-12-21T23:59:35","STAI200201","Completed","2020-10-06T23:59:35","No","No","No","Internal","Will be supplied at next opportunity."]
[null,null,null,14003,null,"48_15/9/2020 2:46:18 PM","2020-08-23T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Kyma computer in ECR not showing aft draft level and log speed.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","11.1","High","","","Receivd spare isolator . Same changed in the panel on the bridge. Tried out. working fine","2020-12-23T23:59:35","","Completed","2020-11-07T23:59:35","No","No","No","Internal"]
[null,null,null,14004,null,"48_15/09/2020 11:55:04 AM","2020-08-27T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Hydro blaster (Combo for high pressure waterjet) not generating sufficient pressure for blasting operation.","Deck - Machinery","General Appearance","Equipment Related","","","","","New spares recd at Singapore on 29June 21. Rotary nozzle attachement tested. Attack holder as well tested and presently system is use. Job completed.","2021-07-21T23:59:35","STAI215026","Completed","2021-06-23T23:59:35","No","No","No","Internal","Any spares required?"]
[null,null,null,14005,null,"48_15/09/2020 11:44:51 AM","2020-08-28T23:59:35","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Engine casing bulkhead which are in shadow of the scrubber room has all turned yellow. Maintenance required for the same.","Miscellaneous","General Appearance","External Factors","","","","","Spot derusting & painting required on funnel casing. Vessel experiencing rolling upto 8deg in Indian ocean. Work aloft to be undertaked when favourable conditions are achived","2020-09-27T23:59:35","","Completed","2020-09-29T23:59:35","No","No","No","Internal"]
[null,null,null,14006,null,"48_17/09/2020 1:30:32 PM","2020-08-28T23:59:35","Other","Owner / Marine / Tech. Suptd.","Ship Staff Insp.","Pump room hatch found with leak stain marks at port side.","Miscellaneous","General Appearance","External Factors","11.6","Medium","","","Derusting & painting of Hatch coaming to be done.","2020-11-21T23:59:35","","Completed","2020-09-16T23:59:35","No","No","No","Internal"]
[null,null,null,14007,null,"48_17/09/2020 1:37:08 PM","2020-08-28T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Ship Staff Insp.","All winches and windlasses gear oil to be checked as some appeared emulsified and above sight glass level.","Deck - Mooring Machinery","Mooring","Equipment Related","9.14","Medium","","","Hydraulic oil renewed for all mooring winches enclosed gears. Sight glass cleaned from inside. Oil level visible clearly in all mooring winches.","2020-11-21T23:59:35","","Completed","2020-11-13T23:59:35","No","No","No","Internal"]
[null,null,null,14009,null,"48_15/9/2020 2:35:44 PM","2020-08-28T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ME turbocharger air suction room to derust and paint","E/R - Aux. Mach.","General Appearance","Equipment Related","10.32","Very High","","","Dresuted . Grit blasted the grating and railing by bringing outside on the Sunken deck. Painted the  grating and the frames and the floor","2020-09-27T23:59:35","","Completed","2020-09-12T23:59:35","No","No","No","Internal"]
[null,null,null,14014,null,"48_15/09/2020 11:47:15 AM","2020-08-28T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Engine room blower casing rust weep marks appearing. To paint or clean using oxalic acid","E/R - Pipes/ valves & fittings","General Appearance","External Factors","10.32","Very High","","","Spot derusting & painting completed. Blower casing washed with oxalic acid. Pics updated in weekly maintenance report","2020-09-27T23:59:35","","Completed","2020-09-02T23:59:35","No","No","No","Internal"]
[null,null,null,14015,null,"48_15/09/2020 11:35:51 AM","2020-08-28T23:59:35","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","HHC manhole door and area below grating to clean / paint.","Miscellaneous","General Appearance","External Factors","","","","","Derusting & painting of HHC manhole 4nos completed. ","2020-09-07T23:59:35","","Completed","2020-09-06T23:59:35","No","No","No","Internal"]
[null,null,null,14016,null,"48_15/09/2020 11:19:56 AM","2020-08-28T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Ladder of masthead at midship rusted.  Maintenance to be carried out","Deck - Pipe / Fittings","General Appearance","External Factors","11.1","High","","","Derusting & painting of ladder completed","2020-09-07T23:59:35","","Completed","2020-09-06T23:59:35","No","No","No","Internal"]
[null,null,null,14017,null,"48_15/9/2020 2:31:38 PM","2020-08-28T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","BWTS Line near the expansion tank covered with salt, it appears while operation it leaks. TO rectify","E/R - Pipes/ valves & fittings","General Appearance","Equipment Related","6.22","Medium","","","BWTS Line near the expansion leaks rectified.","2020-09-07T23:59:35","","Completed","2020-09-04T23:59:35","No","No","No","Internal"]
[null,null,null,14018,null,"48_15/9/2020 2:41:13 PM","2020-08-28T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","DG Exhaust pipe seal pot not having water. To top up water and maintain","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","DG Exhaust pipe seal pot topped up with water.","2020-09-04T23:59:35","","Completed","2020-08-31T23:59:35","No","No","No","Internal"]
[null,null,null,14019,null,"48_15/09/2020 11:15:36 AM","2020-08-28T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Gas alarm for A deck entrance door found active in CCR. ","Miscellaneous","Safety / LSA / FFA","Equipment Related","5.21","Medium","","","Calibration of accommodation fixed gas detection system to be carried out using SPAN gas ","2020-09-03T23:59:35","","Completed","2020-09-03T23:59:35","No","No","No","Internal"]
[null,null,null,14020,null,"48_15/09/2020 11:32:38 AM","2020-08-28T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Water found accumulated in both life boat. To clean dry and to check source of water leak","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.29","High","","","Upon investigation it was found that the gasket for forward pothole on P-side lifeboat & Aft porthole for S-Lifeboat (rubber packing damaged) was leaking slightly ,also it was found that  butterfly nuts securing frame  on window was bent. Repairs carried out on butterfly securing arrangement & tested. No leak observed after repairs","2020-09-07T23:59:35","STAI200217","Completed","2020-09-07T23:59:35","No","No","No","Internal"]
[null,null,null,14021,null,"48_15/9/2020 2:27:42 PM","2020-08-28T23:59:35","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Aux boiler uptake cladding has dislodged","E/R - Pipes/ valves & fittings","General Appearance","Equipment Related","","","","","Aux boiler uptake cladding riveted and repaired","2020-09-12T23:59:35","","Completed","2020-09-07T23:59:35","No","No","No","Internal"]
[null,null,null,14022,null,"48_15/9/2020 2:38:23 PM","2020-08-28T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Aux boiler no 1 main steam stop valve has steam leak, to remove the lagging, locate the leak and rectify","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Valve Bonnet opened. Changed the gasket","2020-09-27T23:59:35","","Completed","2020-09-09T23:59:35","No","No","No","Internal"]
[null,null,null,14023,null,"48_16/9/2020 8:57:40 AM","2020-09-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","No:1 LT cooler sea water inlet line sacrificial flange leak.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.31","Very High","","","No.1 LT cooler sea water inlet line sacrificial  flange renewedwith new spare. All gasket laso replaced with new one.","2020-11-01T23:59:35","","Completed","2020-09-08T23:59:35","No","No","No","Internal"]
[null,null,null,14024,null,"48_16/9/2020 8:59:15 AM","2020-09-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","No:2 LT cooler sea water inlet line sacrificial  flange leak.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.31","Very High","","","No.2 LT cooler sea water inlet line sacrificial  flange renewedwith new spare. All gasket also replaced with new one.","2020-11-01T23:59:35","","Completed","2020-09-08T23:59:35","No","No","No","Internal"]
[null,null,null,14010,null,"48_17/9/2020 4:12:42 PM","2020-09-05T23:59:35","Defect","Ship Staff","Ship Staff Insp.","THE lUBRICATOR VENT IS KEPT OPENED FOR NO. 1 UNIT. IT IS LEAKING THERE ALL THE TIME.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","ME Lubricator oil leak checked for leakage, all flanged for double wall pipe slacked and found Cylinder lubricator No.5 unit checked and fittings leakaged on the copper gasket. Same replaced with new spare gasket. Servo oil Inlet pipe on no.7 unit copper gasket also same replaced with new one. ","2020-12-05T23:59:35","","Completed","2020-10-18T23:59:35","No","No","No","Internal"]
[null,null,null,14161,null,"48_23/9/2020 5:05:04 PM","2020-09-08T23:59:35","Defect","Ship Staff","Ship Staff Insp.","ME AUX BLOWER NO 1 RUNNING INDICATION  IN AMS (ACONIS) IS NOT SHOWING FOUND THAT RELAY CONTACTOR DEFECTIVE.HIMX40 ","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.37","Medium","","","Relay Contactor replaced with new one. Now running indictor is visible in AMS (aconis).","2021-05-08T23:59:35","STAI200218","Completed","2021-02-23T23:59:35","No","No","No","Internal"]
[null,null,null,14011,null,"48_17/9/2020 6:46:54 PM","2020-09-08T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Drinking water Tank outlet valve found not holding.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Drinking water tank made empty. Changed the valve with new","2020-11-08T23:59:35","","Completed","2020-10-29T23:59:35","No","No","No","Internal","Does vessel have spare valve?"]
[null,null,null,14170,null,"48_03/10/2020 4:02:14 PM","2020-09-10T23:59:35","Defect","Ship Staff","Suptd. Insp.","Operating lever for P/room davit faulty. The lever is not resting in neutral position fute faulty mechanish.","Deck - Machinery","ISM Related","Equipment Related","5.2","Very High","","","Operating lever for P/room davit inspected. maintenance carried out. P/room davit operation tested after maintenance, found in good working condition","2020-09-21T23:59:35","","Completed","2020-09-18T23:59:35","No","No","No","Internal"]
[null,null,null,14012,null,"48_19/09/2020 11:19:45","2020-09-10T23:59:35","Defect","Ship Staff","Ship Staff Insp.","The GMT timing in the EGCS panel is 10 mins behind the actual GMT timing.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Changed the GMT timings as per the advise from the maker ","2020-11-10T23:59:35","","Completed","2020-09-16T23:59:35","No","No","No","Internal"]
[null,null,null,14162,null,"48_23/9/2020 12:30:13 PM","2020-09-14T23:59:35","Defect","Ship Staff","Ship Staff Insp.","ME fuel pump no 4 high temprature sensor diffective.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Sensor replaced with new sapre ","2020-12-14T23:59:35","STAI200220","Completed","2020-10-15T23:59:35","No","No","No","Internal"]
[null,null,null,14163,null,"48_26/9/2020 12:19:26 PM","2020-09-17T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Aux CSW pump no.1 suction valve suspected not holding ","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.31","Very High","","","Aux CSW pump no.1 suction vlave checked found in good condition same cleaned. Discharge valve found seat have deep cut same replaced with new spare.","2020-12-17T23:59:35","STAI200221","Completed","2020-10-20T23:59:35","No","No","No","Internal"]
[null,null,null,14164,null,"48_27/9/2020 2:38:43 PM","2020-09-18T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Grey water pump not pumping eventhough it was checked and overhauled how many time and still no success to make it operational.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","6.14","High","","","New complete pump unit fitted in place and tested. ","2021-07-21T23:59:35","STAI 210020","Completed","2021-07-05T23:59:35","No","No","No","Internal","Spares supplied Passing Singapore."]
[null,null,null,14165,null,"48_3/10/2020 2:18:03 PM","2020-09-18T23:59:35","Defect","Ship Staff","Ship Staff Insp.","All top bracing found leaking","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","6.14","High","","","No.1, 2 & 3 Top Bracing units overhauled usinf new sealing rings. Tested. Alignment checked and put in service. No.4 Unit found to be not leaking. Hence only oil renewed and accumaltor charged. Presently all units are in operational condition.","2021-06-21T23:59:35","STAI200224","Completed","2021-06-17T23:59:35","No","No","No","Internal"]
[null,null,null,14168,null,"48_28/9/2020 1:48:42 PM","2020-09-18T23:59:35","Defect","Ship Staff","Ship Staff Insp.","HP Sootblower #4 & 6 for EGB not operational. Not turning and found to be seized","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Both HP Lance No.4 & 6 sootblower removed from place.  Guide bush removed by local heating and hotwork method. New gland packings fitted and unit fitetd in place and tested.Found satisfactory.","2021-06-21T23:59:35","","Completed","2021-04-13T23:59:35","No","No","No","Internal"]
[null,null,null,14166,null,"48_03/10/2020 3:57:59 PM","2020-09-21T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Accommodation fixed gas detection system System Fault alarm is triggered on bridge & E/R. Display is blank & not responding. ","Accommodation","Safety / LSA / FFA","Equipment Related","","","","","Display unit replaced with spare new.","2020-11-21T23:59:35","","Completed","2020-11-05T23:59:35","No","No","No","Internal"]
[null,null,null,14167,null,"48_4/10/2020 2:55:11 PM","2020-09-21T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Thermostat for JCW preheater for Aux DG is not working.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.37","Medium","","","Thermostat replaced with new one and tested. Found satisfactory. Presently in use and all parameters being monitored.","2021-04-22T23:59:35","STAI200225","Completed","2021-03-25T23:59:35","No","No","No","Internal"]
[null,null,null,14169,null,"48_4/10/2020 2:58:28 PM","2020-09-21T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Unable to do EGB soot blow from ECR. \t","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","With the remote support of ACONIS instruction, the DB Tuner was rebooted and system put in service. Tested the sootblow from ECR nad found working satisfactory.","2021-07-06T23:59:35","","Completed","2021-07-05T23:59:35","No","No","No","Internal"]
[null,null,null,14884,null,"48_31/10/2020 8:50:57 AM","2020-10-10T23:59:35","Critical Equipment","Ship Staff","Ship Staff Insp.","Forward whistle found inoperative after vessel experienced bad weather in south china sea. ","Navigation - Others","Navigation","Equipment Related","","","","","Forward whistle motor overhauled, bearings & crankshft renewed with spare available onboard. After installation operation tested of the whistle, found in good working condition","2020-12-09T23:59:35","","Completed","2020-10-19T23:59:35","No","No","No","Internal"]
[null,null,null,14885,null,"48_31/10/2020 8:40:52 AM","2020-10-14T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Oil dripping from STBD windlass operating lever control assembly.","Deck - Machinery","Mooring","Equipment Related","9.14","Medium","","","O-Ring for windlass operating lever renewed & tested. no leaks observed after replacement. Spare O-rings & plugs needs to be ordered for future troubleshooting","2020-10-21T23:59:35","","Completed","2020-10-17T23:59:35","No","No","No","Internal"]
[null,null,null,14886,null,"48_31/10/2020 8:44:17 AM","2020-10-15T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Spring line mooring winch M4 hydraulic oil return line found leaking. It was noted that the pipe was repaired in the past & needs replacement","Deck - Mooring Machinery","Mooring","Equipment Related","9.14","Medium","","","Section of thye return line for hydraulic line replaced with new pipe fabricated onboard.","2020-10-22T23:59:35","","Completed","2020-10-22T23:59:35","No","No","No","Internal"]
[null,null,null,14883,null,"48_06/11/2020 16:21:29","2020-10-25T23:59:35","Defect","Ship Staff","Ship Staff Insp.","EGB soot blower lances are wasted and detached. ","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","HP #5 & 6, LP #1,2,3 &4 lances removed and sootblow pipes replaced with newly fabricated pipes.Holes drilled to specfication and pipes fitted in places.Tested. Found satifactory.","2021-04-24T23:59:35","","Completed","2021-02-26T23:59:35","No","No","No","Internal"]
[null,null,null,15943,null,"48_01/12/2020 10:26:52 PM","2020-10-27T23:59:35","Defect","Ship Staff","Ship Staff Insp.","4 nos COW machines (2nos from 1C & 2nos from 2C COT ) found inoperative or working intermittently during discharging operation at Daxie oil terminal. ","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.34","High","","","4nos of COW machines overhauled (gun unit & driving unit) after removing from the tank. Machies manually tested for smooth movement after overhauling, found in good working condition. ","2020-12-26T23:59:35","","Completed","2020-11-28T23:59:35","No","No","No","Internal"]
[null,null,null,15944,null,"48_27/11/2020 16:59:47","2020-11-19T23:59:35","Defect","Ship Staff","Ship Staff Insp.","GALLEY BEAKING OVEN NO 2 NOT OPRATIONAL ","Accommodation","General Appearance","Equipment Related","11.16","Low","","","Heating coil replaced with new one and baking oven put in service.","2021-05-22T23:59:35","STAI200273","Completed","2021-03-25T23:59:35","No","No","No","Internal"]
[null,null,null,15946,null,"48_30/11/2020 14:33:25","2020-11-19T23:59:35","Defect","Ship Staff","Ship Staff Insp.","SENSOR FOR T/C RPM FOR AUX ENGINE NOT OPERATIONAL","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Removed T/C and fitted the sensor back. Working good","2021-05-23T23:59:35","","Completed","2020-11-23T23:59:35","No","No","No","Internal"]
[null,null,null,15948,null,"48_18/12/2020 01:36:44","2020-11-23T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Spider coupling for Aft and FWD hydraulic pumps ( # 2 ) damaged. Same needs to be replaced","Deck - Machinery","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Spider coupling replaced for No.2 Aft & Fwd hydraulic pumps.","2021-03-28T23:59:35","","Completed","2021-03-24T23:59:35","No","No","No","Internal","3 coupling has been supplied, change at next opportunity."]
[null,null,null,15945,null,"48_03/12/2020 3:14:45 PM","2020-11-24T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","A-Deck Crew laundry washing machine not operational. PCB & Motor found damaged due to water ingress","Accommodation","MLC Related","Equipment Related","11.16","Low","","","New machine received and same fitted back.","2021-02-18T23:59:35","STAI210039","Completed","2021-02-17T23:59:35","No","No","No","Internal"]
[null,null,null,15952,null,"48_18/12/2020 11:00:51 PM","2020-12-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Accommodation fixed gas detection system - Galley air intake sensor faulty (Sensor path blocked)","Accommodation","Safety / LSA / FFA","Equipment Related","","","","","Sensor inspected & cleaned. Path cleared & tested. System in good working condition & no alarm in the system","2021-02-01T23:59:35","","Completed","2020-12-07T23:59:35","No","No","No","Internal"]
[null,null,null,15953,null,"48_15/12/2020 18:19:46","2020-12-05T23:59:35","Defect","Ship Staff","Ship Staff Insp.","EMERGENCY GENERATOR SPRING START STARTER NOT OPERATIONAL.","Critical Equip.","Emgcy. Systems","Equipment Related","10.32","Very High","","","Overhauled the starter. Found one pin broken. same fabricated and tried out.","2020-12-19T23:59:35","STAI200276","Completed","2020-12-07T23:59:35","No","No","No","Internal"]
[null,null,null,15949,null,"48_15/12/2020 17:59:19","2020-12-07T23:59:35","Defect","Ship Staff","Ship Staff Insp.","M/E VISCOSITY NOT SHOWING (SHOWING ZERO) ON CONTROLLER","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Viscocity reading is showing at present after troubleshoot. ","2021-03-22T23:59:35","STAI 210011","Completed","2021-03-23T23:59:35","No","No","No","Internal","RO to be raised in new year for required spares"]
[null,null,null,15950,null,"48_15/12/2020 18:10:24","2020-12-07T23:59:35","Defect","Ship Staff","Ship Staff Insp.","NO 2S COT ullage error in SAAB system. No responce from 2S TGU  unit. ","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.12","Medium","","","CHANGED THE SPARE TGE UNIT. TRIED OUT. WORKING GOOD","2021-03-22T23:59:35","","Completed","2020-12-20T23:59:35","No","No","No","Internal"]
[null,null,null,15951,null,"48_18/12/2020 11:09:05 PM","2020-12-07T23:59:35","Defect","Ship Staff","Ship Staff Insp.","During grit blasting of Hydraulic lines on deck. 3 holes observed in  Hydraulic oil return line for aft mooring winches (Spring lines)","Deck - Pipe / Fittings","Mooring","Equipment Related","11.4","Very High","","","Section of pipe removed & renewed.","2020-12-11T23:59:35","","Completed","2020-12-15T23:59:35","No","No","No","Internal"]
[null,null,null,16514,null,"48_02/01/2021 05:27:40","2020-12-19T23:59:35","Defect","Ship Staff","Ship Staff Insp.","AIR CONDITION COMPRESSOR #1  MOTOR WINDING BURNT","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","New motor recived at Fujiarah and fitted in place. Conenctions made and rotation checked.","2021-05-21T23:59:35","","Completed","2021-03-02T23:59:35","No","No","No","Internal","Motor will be arranged at next opportunity"]
[null,null,null,17555,null,"48_23/01/2021 18:43:47","2020-12-21T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Galley waste overboard pipe holed. Overboard valve not holding","Deck - Pipe / Fittings,E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","11.4","Very High","","","Overboard valve replaced with new one and corroded pipe  replaced with newly fabricated pipe.","2021-03-22T23:59:35","","Completed","2021-03-07T23:59:35","No","No","No","Internal"]
[null,null,null,17556,null,"48_23/01/2021 18:47:54","2020-12-22T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Visco sensor for Generator not showing correct value.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","New spares used to troubleshoot the problem. Presently values are ok and being monitored.","2021-05-22T23:59:35","","Completed","2021-03-23T23:59:35","No","No","No","Internal"]
[null,null,null,17557,null,"48_23/01/2021 1:52:38 AM","2021-01-05T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Pneumatic discharge control valve for AUS system No.3 line in not operating in intermediate position. The valve is operating Open-Shut normally, but unable to maintain intermediate position ","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.8","Medium","","","New Valve positioner fitted in place.Tested. Found operating satisfactorily.","2021-05-21T23:59:35","STAI210044","Completed","2021-04-18T23:59:35","No","No","No","Internal"]
[null,null,null,17682,null,"48_01/02/2021 3:44:00 PM","2021-01-20T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Garbage compactor hydraulic power pack motor burned & hydraulic RAM oil seal leaking","Miscellaneous","MARPOL Related","Equipment Related","6.2","High","","","Spare received will be insatlled after discharge port. New Garbage compactor Installed ","2021-12-21T23:59:35","STAI210038","Completed","2021-11-12T23:59:35","No","No","No","Internal","New compactor supplied already, Need to be installed at first opportunity."]
[null,null,null,17683,null,"48_30/01/2021 19:49:06","2021-01-21T23:59:35","Defect","Ship Staff","Ship Staff Insp.","MGPS main panel power module and display PCB burnt\t\t\t\t\t\t","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.37","Medium","","","MGPS main panel power module fitted with new supplied spare and system put in use.","2021-04-06T23:59:35","STAI210036","Completed","2021-04-06T23:59:35","No","No","No","Internal"]
[null,null,null,17858,null,"48_03/02/2021 4:20:54 PM","2021-01-21T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Observed slight air leaking from AUS gas extraction valve. Suspected O ring damage. ","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.8","Medium","","","All three GEV’s for the AUS system overhauled. Five (5pc) damaged “O” rings replaced with new ones. All moveable components freed and lubricated includding air cylinder mechanism for each units. The system have been tested manually as well as in auto mode and found working smoothly without any internal air leak","2021-03-21T23:59:35","","Completed","2021-01-23T23:59:35","No","No","No","Internal"]
[null,null,null,17856,null,"48_15/02/2021 22:08:05","2021-01-30T23:59:35","Defect","Ship Staff","Ship Staff Insp.","FORWARD HOR NOT WORKING","Navigation - Others","Navigation","Equipment Related","","","","","Complete Air Horn replaced with new one along with motor assembly. Now working satisfactory.","2021-04-29T23:59:35","STAI215007","Completed","2021-02-19T23:59:35","No","No","No","Internal"]
[null,null,null,17857,null,"48_10/02/2021 20:39:28","2021-02-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","ME servo oil filter drain valve not opening on auto.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","ME servo oil fiter drain valve made opeartional.","2021-05-01T23:59:35","STAI200219","Completed","2021-04-17T23:59:35","No","No","No","Internal"]
[null,null,null,17859,null,"48_11/02/2021 8:04:08 PM","2021-02-02T23:59:35","Defect","Ship Staff","Ship Staff Insp.","It was observed that SAAB Tank gauging system Display LCD screen stopped working. Temporary one LCD monitor from training room is being used for SAAB tank gauging display. PO to be raised for new Display","Miscellaneous","Cargo / Ballast Systems","Equipment Related","","","","","Temporary one LCD monitor from training room is being used for SAAB tank gauging display. PO to be raised for new Display","2021-05-01T23:59:35","STAI210053","Completed","2021-02-02T23:59:35","No","No","No","Internal"]
[null,null,null,18197,null,"48_02/03/2021 14:38:08","2021-02-17T23:59:35","Critical Equipment","Ship Staff","Ship Staff Insp.","ER Vent No.1 (S) found erratic during  functional test. Upon checking noticed one end of shaft bearing is worn out and slight play during operation","Critical Equip.","Safety / LSA / FFA","Equipment Related","10.32","Very High","","","The operation of flap found to be opening/closing but there is some extended play at shaft end. Bearing housing dismantled and found bearing completely damaged. No spare available. Brass bush with steel support fabricated and fitted in place. Flap tried out and working satisfactorily. Original bearing unit will be fitted upon receiving new spares.","2021-06-21T23:59:35","STAI210138","Completed","2021-06-17T23:59:35","No","No","No","Internal"]
[null,null,null,18198,null,"48_03-Mar-21 19:10:50","2021-02-17T23:59:35","Defect","Ship Staff","Ship Staff Insp.","No.1 & No.2 MACs antivibartion mounting pads to be renewed as heavy vibrations have been noticed during running. Also, the old vibration mounting pads are totally compressed.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Both Main Air Compressors Anti-Vibration pads replaced with new ones.","2021-04-21T23:59:35","","Completed","2021-03-01T23:59:35","No","No","No","Internal"]
[null,null,null,18977,null,"48_28/04/2021 00:12:36","2021-03-03T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","No.1 Air Con Compressor crankcase inspected and found with broken metal pieces. ","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","All unit cylinder covers opened and cylinders inspected. Found 2nd & 3rd stage unloading mechanism broken. Same overhauled using recently supplied spares. Valve plates and gaskets replaced. Compressor tested.","2021-04-21T23:59:35","","Completed","2021-03-30T23:59:35","No","No","No","Internal"]
[null,null,null,18962,null,"48_15-Apr-21 14:18:41","2021-03-06T23:59:35","Defect","Ship Staff","Ship Staff Insp.","EGB HP & LP Sootblower lance sealing air lines found corroded and clogged inside. Hence only small amount air is sealing the chamber.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","All Sealing Air pipes ( Total HP Lances- 6Nos / LP Lances - 4 nos)  replaced with new fabricated pipes. ","2021-06-21T23:59:35","","Completed","2021-06-14T23:59:35","No","No","No","Internal"]
[null,null,null,18963,null,"48_26/04/2021 23:13:49","2021-03-06T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Service Air  compressor anti-vibration pads are compressed maximum and vibration noticed during starting.\t","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","New anti-vibration pads fitted in place and compressor tested. Found to be satisfactory.","2021-07-21T23:59:35","STAI 210059","Completed","2021-07-15T23:59:35","No","No","No","Internal"]
[null,null,null,19603,null,"48_02/06/2021 6:05:18 PM","2021-03-06T23:59:35","Defect","Ship Staff","Ship Staff Insp.","BWTS NU pumps P132 and P232 are not starting.\n\nAlso tried to change over to manual mode on CCR/LOP screen to start the pump manually however “Start fail” arises.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.8","Medium","","","GC claim raised. Transferred to GC Claim for BWTS","2021-06-30T23:59:35","","Completed","2021-06-22T23:59:35","No","No","No","Internal"]
[null,null,null,19604,null,"48_02/06/2021 6:08:40 PM","2021-03-06T23:59:35","Defect","Ship Staff","Ship Staff Insp.","BWTS Pumproom filter valve BT 1211 is not operating.\n\nMotor fail alarm showing on the valve display unit","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.8","Medium","","","Raised GC claim. Transferred to GC claim Records of BWTS","2021-07-21T23:59:35","","Completed","2021-06-22T23:59:35","No","No","No","Internal"]
[null,null,null,18969,null,"48_15-Apr-21 14:46:41","2021-03-08T23:59:35","Defect","Ship Staff","Ship Staff Insp.","EGCS SCS tracing heater shorted . System switched off as per maker advice.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.11","Medium","","","EGCS SCS new sample  tracing heater fitted in place and system back to normal  with AUTO mode.","2021-05-08T23:59:35","","Completed","2021-04-07T23:59:35","No","No","No","Internal"]
[null,null,null,18970,null,"48_16-Apr-21 16:21:13","2021-03-21T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Twist on the Port side hose handling crane wire, to be freed. ","Deck - Machinery","Cargo / Ballast Systems","Equipment Related","8.5","Very High","","","Remove Twist on the wire","2021-03-27T23:59:35","","Completed","2021-03-21T23:59:35","No","No","No","Internal"]
[null,null,null,18971,null,"48_16-Apr-21 16:28:15","2021-03-21T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Steering gear room davit not moving freely. ","Deck - Machinery","Cargo / Ballast Systems","Human Error","8.63","High","","","Derusting to be carried out and greased on davit","2021-03-31T23:59:35","","Completed","2021-03-25T23:59:35","No","No","No","Internal"]
[null,null,null,18972,null,"48_16-Apr-21 16:30:55","2021-03-21T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Emergency lights stand for lifeboat base rusted- Same to de-rust and grease to apply","LSA / FFA","Safety / LSA / FFA","Human Error","","","","","Derust and grease ","2021-03-26T23:59:35","","Completed","2021-03-23T23:59:35","No","No","No","Internal"]
[null,null,null,18973,null,"48_16-Apr-21 16:34:05","2021-03-21T23:59:35","Non Conformity","Ship Staff","Ship Staff Insp.","Helicopter landing area not painted  with antiskid – Slippery surface","Miscellaneous","Safety / LSA / FFA","Inappropriate Procedure","","","","","Anti skid paints to be applied on helicopter landing area","2021-04-10T23:59:35","","Completed","2021-03-21T23:59:35","No","No","No","Internal"]
[null,null,null,18974,null,"48_16-Apr-21 16:36:07","2021-03-21T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Smoking room bulkheads stained, to be cleaned. ","Accommodation","General Appearance","Behaviour Based,Inappropriate Procedure","","","","","Cleaning required","2021-04-06T23:59:35","","Completed","2021-03-24T23:59:35","No","No","No","Internal"]
[null,null,null,19367,null,"48_04-May-21 12:41:40","2021-03-21T23:59:35","Defect","Ship Staff","Ship Staff Insp.","EGB soot lance LP5 stuck","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Same to be made free","2021-04-01T23:59:35","","Completed","2021-03-30T23:59:35","No","No","No","Internal"]
[null,null,null,19368,null,"48_04/05/2021 15:15:26","2021-03-21T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Hydraulic oil leak from ME servo rail through O- rings of Rail valve for no.3 unit to rectify","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","6.14","High","","","Rail valves O-rings replaced . Tested. No leaks.","2021-03-30T23:59:35","","Completed","2021-03-28T23:59:35","No","No","No","Internal"]
[null,null,null,18960,null,"48_15-Apr-21 14:12:52","2021-03-24T23:59:35","Defect","Ship Staff","Ship Staff Insp.","F.W. Tank outlet valve found not holding when other tank in use. Level rising in gradual manner. ","Hull & Tanks","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","New valve  fitted in place during tank inspection. Job completed satisfactory.","2021-05-21T23:59:35","","Completed","2021-04-25T23:59:35","No","No","No","Internal"]
[null,null,null,19495,null,"48_11/05/2021 22:00:51","2021-03-25T23:59:35","Critical Equipment","Ship Staff","Ship Staff Insp.","Emg Gen spring starter found defective.\t","Critical Equip.","Emgcy. Systems","Equipment Related","10.16","Very High","","","New spring starter recieved at Cape Town and fitted in palce. Tested. Found satisfactory.","2021-05-21T23:59:35","STAI210060","Completed","2021-05-02T23:59:35","No","No","No","Internal"]
[null,null,null,18964,null,"48_15-Apr-21 15:15:00","2021-03-26T23:59:35","Defect","Ship Staff","Ship Staff Insp.","IG O2 analyzer no.2 showing error while on calibrating with span gas.","Inert Gas","Eng. / Strg. Comp.","Equipment Related","8.22","Very High","","","As per the troubleshooting the gas flow has been checked and confirmed ok. The sensor unit has been replaced with spare one still same result. Advice and checks as per makers carried,out still no result. New analyzer unit has been ordered.New O2 analyser recived and same fitted and tried out working satisfactory","2021-07-22T23:59:35","STAI 210106","Completed","2021-06-21T23:59:35","No","No","No","Internal"]
[null,null,null,18975,null,"48_29/04/2021 16:42:46","2021-03-27T23:59:35","Defect","Ship Staff","Ship Staff Insp.","No.1 Air con compressor tripped on over currentwhile testing the system.\t","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Thorough investigation carried out and found magnetic coil along with OCR malfunctioning.Same received at last Singapore call and fitted . System tried out and working satisfactorily.","2021-05-21T23:59:35","","Completed","2021-04-08T23:59:35","No","No","No","Internal"]
[null,null,null,18976,null,"48_15-Apr-21 14:57:38","2021-03-27T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Tank level gauge for no.2 HFO Bunker tank not showing any value.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","8.19","High","","","The dual check type safety chamber opened up and float cleaned, diaphragm checked and found working good. SpareModulator unit has been orderd via PO: STAI210103.","2021-06-26T23:59:35","STAI 210103","Completed","2021-04-20T23:59:35","No","No","No","Internal"]
[null,null,null,19363,null,"48_08/05/2021 13:52:12","2021-03-30T23:59:35","Defect","Ship Staff","Ship Staff Insp.","COPT Mechanical seal leak off alarm barrier defective.","Deck - Machinery","Eng. / Strg. Comp.","Equipment Related","8.1","Very High","","","Upon checking found barrier defective. Found PCB burnt. Spares ordered. Presently system is opeartional as temprory repaire carried out on PCB.","2021-07-06T23:59:35","STAI 210099","Completed","2021-06-16T23:59:35","No","No","No","Internal"]
[null,null,null,18978,null,"48_15-Apr-21 14:24:36","2021-04-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Both FWG Ejector pump discharge valves are not holding and leaking from gland packing.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","New valve fitted in No.2 Pump. No.1 disc valve overhauled and fitted in place. Both pumps tried out and put in use.","2021-05-21T23:59:35","","Completed","2021-04-18T23:59:35","No","No","No","Internal"]
[null,null,null,18965,null,"48_24/04/2021 23:36:07","2021-04-06T23:59:35","Observation","Ship Staff","Ship Staff Insp.","ER Funnel deck plating found corroded  at many places. Hand rail noted completely wasted due to corrosion.","Hull & Tanks","Structural Condn. / WT integrity ","Equipment Related","8.12","Medium","","","ER Funnel deck plating de-rusted completely and painted. ","2021-06-21T23:59:35","STAI 210064","Completed","2021-06-04T23:59:35","No","No","No","Internal"]
[null,null,null,18966,null,"48_29/04/2021 17:51:35","2021-04-09T23:59:35","Defect","Ship Staff","Ship Staff Insp.","No.1 Air con compressor not showing lub oil pressure while running.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","New  controller (complete) and pressure transmitter fitted and system tried out working satisfactory","2021-07-22T23:59:35","STAI 210104","Completed","2021-07-18T23:59:35","No","No","No","Internal","Spares will be supplied in this call Singapore. Target date revised."]
[null,null,null,18967,null,"48_24/04/2021 23:14:50","2021-04-14T23:59:35","Defect","Ship Staff","Ship Staff Insp.","No.2 Aux C.S.W.Pump not building pressure and abnormal noise during running.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Pump dismantled , all aprts cleaned and inspected. Mechanical seal, sleeve and other packings replaced. Pump fitted in place and tested. Found satisfactory.","2021-06-21T23:59:35","","Completed","2021-05-02T23:59:35","No","No","No","Internal"]
[null,null,null,18968,null,"48_29/04/2021 18:00:08","2021-04-18T23:59:35","Defect","Ship Staff","Ship Staff Insp.","MDO Transfer pump suction valve not holding .\t","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Suction line has been isolated by closing the tank outlet valve. Valve dismantled and checked. Found slight damage in seating surface. Same lapped and tested. Found no leaks. Job completed satisfactory.","2021-05-21T23:59:35","","Completed","2021-04-26T23:59:35","No","No","No","Internal"]
[null,null,null,19369,null,"48_08/05/2021 21:16:28","2021-04-24T23:59:35","Observation","Ship Staff","Ship Staff Insp.","NO.1 Drink Water pump shaft seal leaking.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Pump overhauled using new mechanical seal.Tested. Put in service.","2021-05-11T23:59:35","","Completed","2021-04-28T23:59:35","No","No","No","Internal"]
[null,null,null,19364,null,"48_08/05/2021 14:19:23","2021-04-26T23:59:35","Defect","Ship Staff","Ship Staff Insp.","BWTS no.1 main filter for sea water system, pressure transmitter in/out not displaying any value ( zero) on CCR control panel.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","6.21","High","","","BWTS no.1 main filter for sea water system, pressure transmitter in/out not displaying any value ( zero) on CCR control panel.Pressure sensor removed , calibrated and system tried out working satisfactory","2021-05-21T23:59:35","","Completed","2021-05-11T23:59:35","No","No","No","Internal"]
[null,null,null,19365,null,"48_07/05/2021 14:33:41","2021-04-27T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Drink Water Hydrophore tank unit  safety valve not working.","E/R - Aux. Mach.","MLC Related","Equipment Related","10.32","Very High","","","Safety valve removed from place after isolating the Drink wtr hydrophore tank. Valve dismantled and all parts cleaned. Assembled , tested and same fitted in place. Working satisfactorily.","2021-05-21T23:59:35","","Completed","2021-05-05T23:59:35","No","No","No","Internal"]
[null,null,null,19366,null,"48_09/05/2021 23:13:02","2021-04-28T23:59:35","Defect","Ship Staff","Ship Staff Insp.","No.1 Drinking Water Pump impeller in bad condition.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Impeller and casing ring renewed. Pump tried out no abnormal vibrations.","2021-08-21T23:59:35","STAI 210113","Completed","2021-08-19T23:59:35","No","No","No","Internal","Spares will be supplied once ready. Target date revised."]
[null,null,null,19490,null,"48_12/05/2021 22:18:05","2021-05-02T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Valve remote control system pressure switch malfunction","Deck - Machinery","Cargo / Ballast Systems","Equipment Related","8.1","Very High","","","New pressure switch fitted in the VRCS system and same tried out , working satisfactory ","2021-07-21T23:59:35","RO STAI210117","Completed","2021-07-18T23:59:35","No","No","No","Internal","Spares will be supplied in this call Singapore. Target date revised."]
[null,null,null,19491,null,"48_12/05/2021 22:32:32","2021-05-03T23:59:35","Defect","Ship Staff","Ship Staff Insp.","ODME system \"GPS signal fail alarm\"","Deck - Machinery","Cargo / Ballast Systems","Equipment Related","6.1","Medium","","","ODME SYSTEM \"GPS SIGNAL FAIL ALARM\" Appearing on display system while testing the system. GPS output from GPS buffer unit to ODME input found in good order , observed voltage 0.4 to 3.7 vdc , Final adjustments carried out from GPS output sentence and system tried out working satisfcatory","2021-07-06T23:59:35","","Completed","2021-05-29T23:59:35","No","No","No","Internal"]
[null,null,null,19492,null,"48_13/05/2021 04:41:50","2021-05-03T23:59:35","Defect","Ship Staff","Ship Staff Insp.","No.2 IGS Deck Seal pump shaft found broken during running. \t","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Pump dismantled. All parts cleaned. Shaft replaced with old spare one. New mechanical seal and O-ring fitted. Pump tried out.  All parameters are normal. Pump put in service.","2021-05-11T23:59:35","","Completed","2021-05-08T23:59:35","No","No","No","Internal"]
[null,null,null,19493,null,"48_13/05/2021 15:00:42","2021-05-03T23:59:35","Defect","Ship Staff","Ship Staff Insp.","UV Flame detector malfuncton above Aux. Boiler No.1","LSA / FFA","Eng. / Strg. Comp.","Equipment Related","5.3","Low","","","UV Flame detector malfuncton above Aux. Boiler No.1 same dismentaled cleaned and fitted back but after some again malfunction , no spare detector onboard , need to replave with spare. RO STAI210114, Prsently system is working fine ","2021-05-21T23:59:35","RO STAI210114","Completed","2021-05-14T23:59:35","No","No","No","Internal"]
[null,null,null,19494,null,"48_14/05/2021 23:42:21","2021-05-05T23:59:35","Critical Equipment","Ship Staff","Ship Staff Insp.","OWS Carbon filter tank found holed during operation. \t","Critical Equip.","MARPOL Related","Equipment Related","6.17","Very High","","","New Tank fitted in place and all connections given. Leak test carried out. Found satisfactory.","2021-06-21T23:59:35","","Completed","2021-06-10T23:59:35","No","No","No","Internal"]
[null,null,null,19607,null,"48_02/06/2021 16:25:46","2021-05-05T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Suction side distance piece for no.1 SW feed pump for EGCS system got holed.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Same piece removed from place and brought to workshop. Welded and epoxy coated. fitted back in place. System tried out.","2021-05-22T23:59:35","","Completed","2021-05-21T23:59:35","No","No","No","Internal"]
[null,null,null,19606,null,"48_24/05/2021 15:32:11","2021-05-14T23:59:35","Defect","Ship Staff","Engineering Audit","On bridge Signal light and navigation light  control panel  defective","Elect. Mach. & Equip.,Navigation - Others","Communication","Equipment Related","4.7","High","","","Signal light control panel and relay changed. system operation. Navigation light control panel and relay box replaced with spare working satisfactory","2021-09-21T23:59:35","STAI210134","Completed","2021-09-16T23:59:35","No","No","No","Internal","Spares are in capetown, will be connected to vessel in loaded passage."]
[null,null,null,19605,null,"48_30/05/2021 03:54:53","2021-05-20T23:59:35","Defect","Ship Staff","Engineering Audit","M/E OMD system not oprational \" COMMS FAULT \"","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.2","Low","","","M/E OMD system not oprational \" COMMS FAULT \"  for all 9 detectors , all 9 detectors cleaned and fitted back, wiring and power suplly checked found all intact, system in fault further troubleshooting in progress , suspecting issue with interface PCB , RO STAI210126 raised in PAL .Interface PCB replaced with new spare and system tried out working satisfactory","2021-07-21T23:59:35","STAI210126","Completed","2021-06-21T23:59:35","No","No","No","Internal"]
[null,null,null,19725,null,"48_12/06/2021 19:23:57","2021-05-25T23:59:35","Defect","Ship Staff","Engineering Audit","Salino meter For Aux Bolier not operational ","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","During routine alarm testing observed Salino meter and salinity sensor For Aux Bolier are not operational , to rectify same sensor cleaned and salinometer dismentaled cleaned and fitted back , checkes carried out as per manual instructions but no result. To rectify same need to replave with spare RO STAI210128, New recieved spares fitted and system tried out working satisfactory","2021-07-21T23:59:35","STAI210128","Completed","2021-07-14T23:59:35","No","No","No","Internal"]
[null,null,null,19846,null,"48_30/06/2021 20:56:40","2021-06-16T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Both FWG Feed water pipeline (Copper) pin hole.\t\t","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Pipes fabricated and installed.","2021-08-22T23:59:35","STAI210125","Completed","2021-07-26T23:59:35","No","No","No","Internal"]
[null,null,null,19847,null,"48_30/06/2021 21:03:58","2021-06-19T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Main DG2  Fuel Shut off valve Air cylinder leaking.\t","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","During testing of Fuel shut off valve, it was noted that air is leaking from  cylinder top nut. Air cylinder dismantled and found  piston is badly worn out  with no sealing. Hence new piston rod with piston fabricated and fitted in palce. Tested found operarting satisafctory.","2021-07-21T23:59:35","","Completed","2021-06-20T23:59:35","No","No","No","Internal"]
[null,null,null,20039,null,"48_14/07/2021 10:41:35","2021-06-25T23:59:35","Observation","Ship Staff","Ship Staff Insp.","NO.1 ER Vent fan flap / casing found to be corroded inside.","Critical Equip.","Safety / LSA / FFA","Equipment Related","10.27","Medium","","","Blower casing removed from place, de0rusted completely and applied with two coats of epoxy paints followed by final one. Same fitted in place and tested. Found satisfactory.","2021-07-21T23:59:35","","Completed","2021-07-02T23:59:35","No","No","No","Internal"]
[null,null,null,20660,null,"48_29/08/2021 4:12:21 PM","2021-07-11T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","The emergency light casing on bridge wing - port side aft (next to the elevator access hatch) had water collected.","Accommodation","Emgcy. Systems","Equipment Related","11.9","Low","","","Collected water removed from the the emergency light casing","2021-08-10T23:59:35","","Completed","2021-07-12T23:59:35","No","No","No","Internal"]
[null,null,null,20661,null,"48_29/08/2021 4:34:11 PM","2021-07-11T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","VDR Fixed Protective Capsule Unit on monkey island - The expiry date for battery is stencilled as Oct-2022, however on the battery expiry is indicated as Jul-2024.","Navigation - VDR / BNWAS","Navigation","Human Error","","","","","Stencil renewed expiry date as July 2024","2021-07-22T23:59:35","","Completed","2021-07-20T23:59:35","No","No","No","Internal"]
[null,null,null,20662,null,"48_29/08/2021 4:41:51 PM","2021-07-11T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","The grab lines for the port side M.O.B Marker appeared to be old.","LSA / FFA","Safety / LSA / FFA","External Factors","5.3","Low","","","Grab line of M.O.B marker renewed.","2021-08-22T23:59:35","","Completed","2021-07-27T23:59:35","No","No","No","Internal"]
[null,null,null,20154,null,"48_27/07/2021 11:12:37","2021-07-11T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Incinerator display is faded to renew.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Spare received,installed. Incinerator tried out. working satisfactory.","2021-09-21T23:59:35","RO STAI210183","Completed","2021-10-08T23:59:35","No","No","No","Internal","Spare on order. Will be connected at convenient port. target date revised."]
[null,null,null,20156,null,"48_22/07/2021 7:02:42 PM","2021-07-11T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Funnel area Stbd side door rain protector wasted. To be renewed","Miscellaneous","General Appearance","External Factors,Industry Issue","11.6","Medium","","","Wasted rain protector to be renewed","2021-08-01T23:59:35","","Completed","2021-07-21T23:59:35","No","No","No","Internal"]
[null,null,null,20157,null,"48_22/07/2021 8:05:37 PM","2021-07-11T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Stbd Lifeboat few glasses are already faded and Opaque. Needs to be renewed.","LSA / FFA","Safety / LSA / FFA","External Factors","5.29","High","","","Spares received, will installed after discharge port. Life boat glass renewed ","2021-10-21T23:59:35","STAI210186","Completed","2021-10-20T23:59:35","No","No","No","Internal","Understand spare received in singapore. Renew at the earliest opportunity."]
[null,null,null,20159,null,"48_22/07/2021 8:15:27 PM","2021-07-11T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Hydraulic box  one side plate near Port side manifold is wasted. To be repaired by bolting arrangement.","Deck - Pipe / Fittings","General Appearance","External Factors","11.4","Very High","","","Wasted area fabricated with new plate and re painted ","2021-07-27T23:59:35","","Completed","2021-07-20T23:59:35","No","No","No","Internal"]
[null,null,null,20160,null,"48_22/07/2021 8:18:18 PM","2021-07-11T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Various supports on deck getting rusty and causing rust weep marks on deck. To be hydroblasted and painted.","Deck - Pipe / Fittings","General Appearance","External Factors","11.4","Very High","","","Derusting and Painting Completed","2021-09-21T23:59:35","","Completed","2021-09-18T23:59:35","No","No","No","Internal","target date revised as per vessel's request."]
[null,null,null,20161,null,"48_27/07/2021 11:09:46","2021-07-11T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Sewage treatment plant blower running indicator is not working.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","lamp replaced with spare working satisfactory","2021-07-21T23:59:35","","Completed","2021-07-12T23:59:35","No","No","No","Internal"]
[null,null,null,20162,null,"48_23/07/2021 14:22:46","2021-07-11T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ME NO.1 & 2  T/C Air inlet manometer found without water","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Manometer removed, cleaned and water filled. Now water level visible.","2021-07-16T23:59:35","","Completed","2021-07-13T23:59:35","No","No","No","Internal"]
[null,null,null,20163,null,"48_22/07/2021 6:58:27 PM","2021-07-11T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Stbd Lifeboat engine exhaust pipe to repair / renew","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.29","High","","","New Exhaust pipe fabricated as per the size and shape. Same fitted in place.","2021-07-22T23:59:35","","Completed","2021-07-19T23:59:35","No","No","No","Internal"]
[null,null,null,20164,null,"48_22/07/2021 6:54:10 PM","2021-07-11T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Slop heating valve manifold to paint","Deck - Pipe / Fittings","General Appearance","External Factors","11.4","Very High","","","De rusting and painting carried out.","2021-07-27T23:59:35","","Completed","2021-07-18T23:59:35","No","No","No","Internal"]
[null,null,null,20165,null,"48_22/07/2021 7:31:13 PM","2021-07-11T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Securing clamp of renewed mooring line is missing at two locations.","Deck - Machinery","Mooring","Inappropriate Procedure","11.5","Medium","","","Installed new U clamps on mooring lines","2021-07-27T23:59:35","","Completed","2021-07-19T23:59:35","No","No","No","Internal"]
[null,null,null,20166,null,"48_22/07/2021 8:08:48 PM","2021-07-11T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Remote control wire end connected to the counterweight at Port side lifeboat canopy needs to be adjusted so that it should not get stuck at the sheave while lowering.","LSA / FFA","Safety / LSA / FFA","Equipment Related,Inappropriate Procedure","5.29","High","","","Adjusted wire of counterweight length -Self lowering wire","2021-07-21T23:59:35","","Completed","2021-07-19T23:59:35","No","No","No","Internal"]
[null,null,null,20167,null,"48_22/07/2021 7:39:22 PM","2021-07-11T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Greasing point of both lifeboat davits are to be highlighted by yellow mark.","Miscellaneous","General Appearance","Inappropriate Procedure","11.3","Medium","","","Highlight greasing points with Yellow paints","2021-07-27T23:59:35","","Completed","2021-07-17T23:59:35","No","No","No","Internal"]
[null,null,null,20153,null,"48_22/07/2021 8:26:29 PM","2021-07-13T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Internal leakage alarm pops up on fixed gas detection for WBT/Pumproom.","Miscellaneous","Safety / LSA / FFA","Equipment Related","8.46","Very High","","","Detailed troubleshooting carried out as per makers insturctions , presently system running without any alarm ","2021-09-20T23:59:35","","Completed","2021-09-05T23:59:35","No","No","No","Internal","Trouble shooting in progress. Target date revised."]
[null,null,null,20155,null,"48_25/07/2021 12:53:27","2021-07-16T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Hydroblaster not operational\t","Deck - Machinery","General Appearance","Equipment Related","","","","","New breaker fitted on to hydroblaster starting panel.","2021-09-21T23:59:35","","Completed","2021-07-24T23:59:35","No","No","No","Internal"]
[null,null,null,20370,null,"48_08/08/2021 21:01:36","2021-07-21T23:59:35","Observation","Ship Staff","Ship Staff Insp.","ME FO Viscosity controller inoperational","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","New controller received, and same fitted in place .System checked, controller responding as per signal","2021-11-21T23:59:35","","Completed","2021-10-27T23:59:35","No","No","No","Internal","Understand presently it is working fine and is under observation."]
[null,null,null,20373,null,"48_12/08/2021 19:13:44","2021-07-21T23:59:35","Observation","Ship Staff","Ship Staff Insp.","ME Unit #4 combustion pressure inidacting sensor not working.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Sensor replaced. Working satisfactory.","2021-11-21T23:59:35","","Completed","2021-08-18T23:59:35","No","No","No","Internal"]
[null,null,null,20374,null,"48_08/08/2021 21:13:50","2021-07-21T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Positioner for EGCS scrubber discharge valve not working","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","New positioner received, installed, System working satisfactory.","2021-11-12T23:59:35","STAI210189","Completed","2021-10-13T23:59:35","No","No","No","Internal"]
[null,null,null,20375,null,"48_08/08/2021 21:36:57","2021-07-21T23:59:35","Observation","Ship Staff","Ship Staff Insp.","ME Unit #1 exhaust valve stroke reading incorrect","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Valve stroke sensor replaced. working good.","2021-11-11T23:59:35","STAI210182","Completed","2021-10-11T23:59:35","No","No","No","Internal"]
[null,null,null,20376,null,"48_12/08/2021 19:23:29","2021-07-21T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Thrust bearing sensor, Local and Remote readings are not matching","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Sensor replaced with spare","2021-11-21T23:59:35","","Completed","2021-10-14T23:59:35","No","No","No","Internal"]
[null,null,null,20377,null,"48_13/08/2021 21:48:08","2021-07-21T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Aux DG cannot be started from ECR","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Mechanical fuel limiter adjusted to 50%of load and lambda controller to 10mm as per maker's instruction.","2021-11-21T23:59:35","STAI210119","Completed","2021-08-23T23:59:35","No","No","No","Internal"]
[null,null,null,20378,null,"48_13/08/2021 21:53:26","2021-07-21T23:59:35","Defect","Ship Staff","Ship Staff Insp.","drinking water fountain in the E/R is not cooling\t","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","New fountain received,installed  working good","2021-11-21T23:59:35","","Completed","2021-10-11T23:59:35","No","No","No","Internal"]
[null,null,null,20379,null,"48_15/08/2021 17:01:19","2021-07-21T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Insulation is low for Baking oven","Elect. Mach. & Equip.","General Appearance","Equipment Related","10.38","Medium","","","Spares received.installed, working satisfactory.","2021-11-21T23:59:35","STAI210199","Completed","2021-10-07T23:59:35","No","No","No","Internal"]
[null,null,null,20384,null,"48_08/08/2021 21:05:41","2021-07-21T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Leaking from coupling of HFO Purifier feed pump #1","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Coupling replaced with new spare.","2021-08-01T23:59:35","","Completed","2021-07-27T23:59:35","No","No","No","Internal"]
[null,null,null,20380,null,"48_12/08/2021 22:08:24","2021-08-03T23:59:35","Observation","Ship Staff","Ship Staff Insp.","No ear clamps for Oxygen/acetylene hoses","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","5.26","Medium","","","All jubilee clips replaced with earclamps.","2021-11-21T23:59:35","STAI215046","Completed","2021-10-10T23:59:35","No","No","No","Internal"]
[null,null,null,20381,null,"48_15/08/2021 17:05:09","2021-08-04T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Window Wiper Stbd. side not operational","Navigation - Others","Navigation","Equipment Related","12.1","High","","","Belt renewed.Wiper operational","2021-11-21T23:59:35","STAI210200","Completed","2021-10-31T23:59:35","No","No","No","Internal","Spares will be arranged in this call Singapore."]
[null,null,null,20383,null,"48_15-Aug-21 14:42:13","2021-08-05T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Gas Measuring instrument Impact Pro not in use due to battery addapter damaged. ","Miscellaneous","Cargo / Ballast Systems","Equipment Related","5.23","Very High","","","Battery addapter received instrument calibrated and found working.  ","2021-10-06T23:59:35","STAI210201","Completed","2021-10-06T23:59:35","No","No","No","Internal"]
[null,null,null,20663,null,"48_20/08/2021 14:03:42","2021-08-07T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Aft air horn malfunctioing.","Navigation - Others","Navigation","Equipment Related","","","","","Air horn unit overhauled.System working.","2021-09-01T23:59:35","STAI210203","Completed","2021-08-11T23:59:35","No","No","No","Internal"]
[null,null,null,20655,null,"48_27/08/2021 19:11:14","2021-08-14T23:59:35","Critical Equipment","Ship Staff","Ship Staff Insp.","BNWAS showing false alarm for the ECDIS and gyro failure","Navigation - VDR / BNWAS","Navigation","Equipment Related","4.7","High","","","Spare IO module recived same renewed and system tried out working satisfactory","2021-09-21T23:59:35","STAI215050.","Completed","2021-09-16T23:59:35","No","No","No","Internal","Sapres will be supplied in Capetown."]
[null,null,null,20656,null,"48_27/08/2021 19:16:55","2021-08-16T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Space heater control circuit for different motors not operational","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Timers renewed, space heaters working satisfactory.","2021-11-21T23:59:35","STAI210206","Completed","2021-10-29T23:59:35","No","No","No","Internal","Spares supplied in Singapore already. Complete the jobs ASAP. Target date revised accordingly."]
[null,null,null,20657,null,"48_26/08/2021 19:21:08","2021-08-17T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Galley AC Controler eratic readings and malfunction","Elect. Mach. & Equip.","General Appearance","Equipment Related","","","","","Spare recived, Same replaced and tried out working satisfactory","2021-10-21T23:59:35","RO STAI210205","Completed","2021-10-12T23:59:35","No","No","No","Internal","Spares received in Singapore. TO be attended."]
[null,null,null,20814,null,"48_06/09/2021 21:01:58","2021-08-27T23:59:35","Observation","Ship Staff","Engineering Audit","ACCONIS External Extension  alarm system for spare cabin acknowledge button not operational ","Elect. Mach. & Equip.","Communication","Equipment Related","10.37","Medium","","","ACCONIS External Extension  alarm system for spare cabin acknowledge button not operational  As agreed with office, this RO was cancelled and shall be raised at later stage, as this is not effecting any operation.","2021-10-21T23:59:35","STAI210215","Completed","2021-09-19T23:59:35","No","No","No","Internal"]
[null,null,null,20815,null,"48_06/09/2021 21:05:39","2021-08-27T23:59:35","Defect,Observation","Ship Staff","Engineering Audit","Main AC no 2 not operational due to  PCB overheat","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.37","Medium","","","Main AC  PCB received installed, AC started working satisfactory.","2021-10-21T23:59:35","STAI210214","Completed","2021-10-07T23:59:35","No","No","No","Internal"]
[null,null,null,20816,null,"48_15/09/2021 00:54:25","2021-08-30T23:59:35","Observation","Ship Staff","Ship Staff Insp.","ME JCW Preheater steam outlet valve leaking","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Bonnet gasket replaced.System in use no leaks.","2021-11-11T23:59:35","","Completed","2021-10-15T23:59:35","No","No","No","Internal"]
[null,null,null,20817,null,"48_14/09/2021 18:17:34","2021-09-05T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Contol panel for #1 HFO purifer broken","E/R - Purifier","Eng. / Strg. Comp.","Equipment Related","10.3","Medium","","","Contol panel for HFO purifer recieved,Installed Purifier tested working satisfactory.","2021-12-21T23:59:35","STAI210219","Completed","2021-10-08T23:59:35","No","No","No","Internal"]
[null,null,null,20818,null,"48_15/09/2021 00:51:48","2021-09-05T23:59:35","Defect","Ship Staff","Ship Staff Insp.","T/G vacuum pump #2 Coupling on motor side found wear down.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Coupling, coupling ring replaced","2021-12-21T23:59:35","STAI210220","Completed","2021-10-30T23:59:35","No","No","No","Internal","Coupling as per RO will be supplied once ready."]
[null,null,null,21283,null,"48_30/09/2021 15:31:44","2021-09-07T23:59:35","Critical Equipment","Ship Staff","Ship Staff Insp.","FIRE DETECTION SYSTEM FAULT CODE 180 MAINS POWER FAULT","Critical Equip.,Elect. Mach. & Equip.","Safety / LSA / FFA","Equipment Related","5.35","Medium","","","Technician attended, replaced charger module.","2021-12-21T23:59:35","STAI215052","Completed","2021-10-25T23:59:35","No","No","No","Internal","Service engineer will be attending in Singapore."]
[null,null,null,20372,null,"48_08/08/2021 21:21:00","2021-09-20T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Contol panel for #2 HFO purifer broken","E/R - Purifier","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Panel replaced","2022-01-22T23:59:35","STAI210061","Completed","2022-01-18T23:59:35","No","No","No","Internal","Spares not yet ready to be supplied. at next port. TArget date revised accordingly."]
[null,null,null,20371,null,"48_08/08/2021 21:11:29","2021-09-21T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Aux Engine proximity switch for Jet assist broken.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Proximity sensor replaced.","2022-01-21T23:59:35","STAI210119","Completed","2022-01-18T23:59:35","No","No","No","Internal","Awaiting readiness."]
[null,null,null,20659,null,"48_28/08/2021 14:28:42","2021-09-27T23:59:35","Observation","Ship Staff","Ship Staff Insp.","MAIN SWITCHBOARD EXTERNAL OPERATING HANDLE MODEL TFH-12NE NOT OPERATIONAL","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.37","Medium","","","MCB REPLACED WITH NEW SPARE","2022-01-21T23:59:35","STAI210216","Completed","2022-01-12T23:59:35","No","No","No","Internal","Spares are on order and awaiting readiness. Target date revised accordingly."]
[null,null,null,18961,null,"48_15-Apr-21 15:07:57","2021-09-28T23:59:35","Defect","Ship Staff","Ship Staff Insp.","ME flowmeter found not showing any reading.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","New flowmeter installed.","2022-01-21T23:59:35","STAI 210204","Completed","2022-01-17T23:59:35","No","No","No","Internal","Sensor will be ready by Nov 2021. Target date revised accordingly."]
[null,null,null,20382,null,"48_08/08/2021 21:17:21","2021-10-04T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Pressure switch for floatation tank malfunctioing","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Replaced with spare pressure switch","2022-03-19T23:59:35","STAI210188","Completed","2022-03-30T23:59:35","No","No","No","Internal"]
[null,null,null,20158,null,"48_22/07/2021 7:25:21 PM","2021-10-11T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Personnel basket to be renewed as same is more than 5 year old.","Miscellaneous","Safety / LSA / FFA","Inappropriate Procedure","5.47","Medium","","","Spare basket received at Singapore on 3rd April 2022","2022-03-19T23:59:35","STAI215043","Completed","2022-03-25T23:59:35","No","No","No","Internal"]
[null,null,null,22220,null,"48_20/10/2021 15:21:18","2021-10-11T23:59:35","Defect","Ship Staff","Ship Staff Insp.","WHRS two temperature of LP TAH #13,TAH #14  side sensor not working","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Sensors replaced with spares recived.","2022-02-19T23:59:35","STAI210261","Completed","2022-01-22T23:59:35","No","No","No","Internal","Spares will be supplied once ready."]
[null,null,null,22221,null,"48_22/10/2021 23:07:32","2021-10-12T23:59:35","Observation","Ship Staff","Ship Staff Insp.","IG Main deck valve leaking","Inert Gas","Cargo / Ballast Systems","Equipment Related","8.25","Very High","","","Actuator installed properly, valve is closing completely. Valve was removed,found seat ring intact","2021-12-21T23:59:35","STAI210262","Completed","2021-11-01T23:59:35","No","No","No","Internal","Will be supplied once ready."]
[null,null,null,22222,null,"48_31/10/2021 15:32:30","2021-10-14T23:59:35","Defect","Ship Staff","Ship Staff Insp.","OIl leaking from Stbd. windlass brake when put to use.","Deck - Mooring Machinery","Mooring","Equipment Related","11.5","Medium","","","opened up the top cover. Renewed the seals. still leaking. ordered for brake screw. Hydraulic cylinder removed and repaired, leak arrested .","2022-01-22T23:59:35","STAI210263","Completed","2021-10-30T23:59:35","No","No","No","Internal","Needs to dismantle and inspect the brake screw area for pitting."]
[null,null,null,20658,null,"48_27/08/2021 19:21:39","2021-10-18T23:59:35","Defect","Ship Staff","Ship Staff Insp.","MAIN ENGINE top bracing solenoide coil  not operational","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Solenoid coil replaced with spare","2022-01-22T23:59:35","STAI210207","Completed","2022-01-11T23:59:35","No","No","No","Internal","Will be supplied in next call Singapore. Target date revised."]
[null,null,null,22608,null,"48_15-Nov-21 19:22:13","2021-10-26T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Aft winch hydraulic pipe to renew","Deck - Mooring Machinery","Mooring","Equipment Related","9.14","Medium","","","Pipe section removed fabrication in progress. New pipe line fabricated and replaced. Pipe tested all found in good Condition.","2021-11-29T23:59:35","","Completed","2021-11-12T23:59:35","No","No","No","Internal","Understand job is in progress. Target date revised accordingly."]
[null,null,null,22609,null,"48_15-Nov-21 19:42:51","2021-10-26T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Fwd hydraulic cooler SW inlet pipe is fitted temporarily","Deck - Mooring Machinery","General Appearance","Equipment Related","11.4","Very High","","","Permanent pipe to be made and painted.","2021-11-21T23:59:35","","Completed","2021-11-05T23:59:35","No","No","No","Internal","Attend the job ASAP. Target date revised."]
[null,null,null,22610,null,"48_15-Nov-21 19:49:43","2021-10-26T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","The balance grating of deck to be replaced with fiber grating. Understand fiber grating already received.","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.5","Medium","","","Gratings changed","2021-12-06T23:59:35","","Completed","2021-12-01T23:59:35","No","No","No","Internal","I believe vessel has received  the balance gratings"]
[null,null,null,22612,null,"48_15-Nov-21 14:09:47","2021-10-26T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Air ejector steam condesnate return line steam trap bypass valve leaking","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","valve changed","2021-11-11T23:59:35","","Completed","2021-10-31T23:59:35","No","No","No","Internal"]
[null,null,null,22613,null,"48_15-Nov-21 14:14:56","2021-10-26T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ME Auto back wash filter leaking from top seal. .","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","x ring and O' ring changed. leak rectified","2021-11-05T23:59:35","","Completed","2021-10-31T23:59:35","No","No","No","Internal"]
[null,null,null,22614,null,"48_15-Nov-21 14:19:06","2021-10-26T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Gangway angle indicator is fitted wrongly. ","Deck - Pipe / Fittings","General Appearance","Inappropriate Procedure","5.47","Medium","","","corrected and permanent fixture done","2021-11-05T23:59:35","","Completed","2021-11-03T23:59:35","No","No","No","Internal"]
[null,null,null,22615,null,"48_15-Nov-21 14:21:03","2021-10-26T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","IG deck seal gauge glass is not clear","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.23","Medium","","","glass cleaned and put back","2021-11-05T23:59:35","","Completed","2021-11-03T23:59:35","No","No","No","Internal"]
[null,null,null,22616,null,"48_15-Nov-21 14:16:51","2021-10-26T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Air ejector steam inlet valve  leaking.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","valve changed with new","2021-11-15T23:59:35","","Completed","2021-10-31T23:59:35","No","No","No","Internal"]
[null,null,null,22617,null,"48_15-Nov-21 19:46:03","2021-10-26T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","The loop of the metal plate installed on bridge wing is corroded and missing. To repair","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.5","Medium","","","Loop  on the metal plate fabricated, painted and put back in place.","2021-11-05T23:59:35","","Completed","2021-11-05T23:59:35","No","No","No","Internal"]
[null,null,null,22618,null,"48_15-Nov-21 19:35:37","2021-10-26T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Engine room davit pipe completely corroded","Deck - Pipe / Fittings","General Appearance","Equipment Related","10.29","Medium","","","Pipe replaced.","2021-11-10T23:59:35","","Completed","2021-11-06T23:59:35","No","No","No","Internal"]
[null,null,null,22611,null,"48_15-Nov-21 19:53:15","2021-11-02T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Accomdation gas sampling system Galley intake flow failure fault","Accommodation","Safety / LSA / FFA","Equipment Related","5.2","Very High","","","Service engineer attended vessel.","2022-02-11T23:59:35","STAI210269","Completed","2022-03-02T23:59:35","No","No","No","Internal","Understand it is already fixed. Then why is it open?"]
[null,null,null,22755,null,"48_01-Dec-21 04:44:26","2021-11-07T23:59:35","Observation","Ship Staff","Ship Staff Insp.","EGCS MGPS AL anode  PCB not operational","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.38","Medium","","","PCB replaced","2022-02-11T23:59:35","STAI210266","Completed","2022-01-15T23:59:35","No","No","No","Internal","Spares are in Singapore and will be connected at next opportunity."]
[null,null,null,22756,null,"48_30-Nov-21 03:56:57","2021-11-16T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Galley waste dispenser seal leaking.","Accommodation","MARPOL Related","Equipment Related","6.2","High","","","Seal to change. Same opened on receipt of spare seal. Vsl found that impeller casing and other parts are wasted and worn out. On telecon with office end same were ordered again. will be replaced on the receipt of the same.\nSpare parts received, Galley waste disposer overhauled and tried out, found working satisfactory","2022-07-13T23:59:35","STAI220079","Completed","2022-05-15T23:59:35","No","No","No","Internal","Spares will be arranged once ready."]
[null,null,null,22757,null,"48_28-Nov-21 05:25:32","2021-11-18T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Ballast Valve BA019 is in 10% open Condition.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.11","Medium","","","During loading operations, valve was operated. And found that valve is closing fully. Probably something was stuck in the seat. Confirmed the operation of valve after making entry into the Tank","2022-01-18T23:59:35","","Completed","2021-12-05T23:59:35","No","No","No","Internal","Does this valve causing any operational issue? Are seat rings available for this valve"]
[null,null,null,22758,null,"48_28-Nov-21 05:42:11","2021-11-18T23:59:35","Defect","Ship Staff","Ship Staff Insp.","COP Seprator No3 level guage Showing Incorrect reading.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.13","Medium","","","COP Seprator Guage Line  Blown through and checked . Gauge showing correct reading now","2022-01-19T23:59:35","STAI210266","Completed","2021-12-04T23:59:35","No","No","No","Internal","Revert after clearing the line."]
[null,null,null,23192,null,"48_22-Dec-21 17:23:49","2021-11-25T23:59:35","Defect","Ship Staff","Ship Staff Insp.","#1 Air conditioing compressor suction gas temperature sensor erratic.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Sensor needs to be replaced. Spares awaited. Will be replaced on receipt of the same.\nNew sensor received and renewed. System operational","2022-07-21T23:59:35","STAI220030","Completed","2022-05-18T23:59:35","No","No","No","Internal"]
[null,null,null,23190,null,"48_22-Dec-21 17:26:17","2021-11-27T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Lathe machine high speed gear damaged, not engaging with driving shaft.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Gear to be changed. Gears were replaced by new spares received at Singapore on 20th FEB 2022.Same tried and tested well. Same to be closed out.","2022-02-25T23:59:35","STAI220031","Completed","2022-02-11T23:59:35","No","No","No","Internal"]
[null,null,null,23193,null,"48_22-Dec-21 17:28:42","2021-12-05T23:59:35","Defect","Ship Staff","Ship Staff Insp.","No1(S) and No 4 (S) Water Ballast Tank Level Guage showing incorrect reading.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.23","Medium","","","sensor checked, found not working. Needs to replace. Spares are on order. Same will be rectified at suitable anchorage.\nSensor received and renewed, system operational\n","2022-07-05T23:59:35","STAI220004","Completed","2022-06-24T23:59:35","No","No","No","Internal"]
[null,null,null,23305,null,"48_31-Dec-21 16:22:13","2021-12-07T23:59:35","Observation","Ship Staff","Ship Staff Insp.","HP Circulating pump #2 under performing","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Pump dismantled, found impller holed, and mouth ring excessive wear down.Needs to replace impellerand wear ring. Awaiting for spares. Same will be overhauled on receipt of the same.\nSpares received, pump overhauled with new impeller in place, pump tested and found working satisfactory","2022-07-11T23:59:35","STAI220023","Completed","2022-06-16T23:59:35","No","No","No","Internal"]
[null,null,null,23306,null,"48_01-Jan-22 22:49:55","2021-12-08T23:59:35","Observation","Ship Staff","Ship Staff Insp.","UV Sterlizer Quartz sleeve broken","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","Replace quratz sleev with spare. Same will be replaced on receipt of the same.\nNew quartz sleeve received and renewed. System tested and operational.","2022-05-22T23:59:35","STAI220025","Completed","2022-06-10T23:59:35","No","No","No","Internal"]
[null,null,null,23307,null,"48_01-Jan-22 23:05:47","2021-12-08T23:59:35","Observation","Ship Staff","Ship Staff Insp.","FWD ICCP Touch screen computer controller display faded","Hull & Tanks","Structural Condn. / WT integrity ","Equipment Related","","","","","need to change display module. Same will be replaced on receipt of the spare.\n\nNew display received and renewed.","2022-06-29T23:59:35","STAI220026","Completed","2022-05-12T23:59:35","No","No","No","Internal"]
[null,null,null,23308,null,"48_01-Jan-22 23:16:30","2021-12-11T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Aux DG Fueloil leak off alarm sensor inoperational.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Sensor needs to replace. Same will be replaced on receipt of the spare.\nSensor received and renewed, tested found working satisfactory.","2022-07-11T23:59:35","STAI220027","Completed","2022-05-14T23:59:35","No","No","No","Internal"]
[null,null,null,23309,null,"48_31-Dec-21 09:52:51","2021-12-15T23:59:35","Defect","Ship Staff","Ship Staff Insp.","FWD Mast Floodlight for STBD windlass heavily corroded","Miscellaneous","Navigation","External Factors","11.9","Low","","","Spares received and lights changed","2022-10-23T23:59:35","STAI 220034","Completed","2022-10-06T23:59:35","No","No","No","Internal","Please complete in good weather condition as planned"]
[null,null,null,23553,null,"48_12-Jan-22 14:58:20","2021-12-24T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Officer's messroom drinkingwater fountain inoperationa","Accommodation","MLC Related","Equipment Related","","","","","New cooler received and replaced","2022-03-05T23:59:35","STAI220014","Completed","2022-01-11T23:59:35","No","No","No","Internal"]
[null,null,null,23554,null,"48_14-Jan-22 22:49:35","2021-12-27T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Turbogenerator Tachotransmitter inoperational. ","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Needs to replace. Same will be replaced on receipt of the spare.\nNew tachmeter received and renewed.","2022-07-05T23:59:35","STAI220038","Completed","2022-06-08T23:59:35","No","No","No","Internal"]
[null,null,null,23963,null,"48_07/02/2022 5:29:20 PM","2022-01-05T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Fore Peak Ballst Vent head float damaged ","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","Equipment Related","","","","","Need to replace the float with new Float. Same replaced with received spare on 25th FEB 2022. Job to be closed out.","2022-05-04T23:59:35","STAI220065","Completed","2022-02-16T23:59:35","No","No","No","Internal"]
[null,null,null,28600,28137,"48_Wed Feb 01 2023 19:39:25 GMT+0800","2022-01-16T23:59:35","Defect","Ship Staff","Ship Staff Insp.","#2 Main Air Compressor leaking from shaft seal ","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","#2 MAC shaft seal replaced with new spare","2023-02-07T23:59:35","","Completed","2023-01-27T23:59:35","No","No","No","Internal"]
[null,null,null,23966,null,"48_10-Feb-22 15:23:01","2022-01-21T23:59:35","Observation","Ship Staff","Ship Staff Insp.","EGCS MGPS Aluminum anode inperational.Anode consumed 40-50%","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Replaced anode in DD.","2022-11-07T23:59:35","STAI220062","Completed","2022-11-28T23:59:35","No","No","No","Internal","complete as planned. we can run down the anodes to 25% and maximize utilization."]
[null,null,null,23964,null,"48_04/02/2022 11:17:29 AM","2022-01-25T23:59:35","Other","Ship Staff","Ship Staff Insp.","Slop (P) tank Radar guage not operational.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.23","Medium","","","RADAR Guage transmiter to be checked. Same will be replaced and rectified on receipt of the spare.\nNew transmitter received and renewed. System operational","2022-04-23T23:59:35","STAI220076","Completed","2022-05-22T23:59:35","No","No","No","Internal"]
[null,null,null,23965,null,"48_04/02/2022 11:56:24 AM","2022-01-25T23:59:35","Observation","Ship Staff","Mooring Audit","Various Hydraulic pipelines on Mooring winch and windlass corroded ","Deck - Mooring Machinery","Mooring","External Factors","9.14","Medium","","","All Corroded pipe need replacement. Same will be replaced and rectified on receipt of the spare.\nPipe renewal carried out","2022-04-23T23:59:35","STAI220066","Completed","2022-06-14T23:59:35","No","No","No","Internal"]
[null,null,null,23967,null,"48_09-Feb-22 19:50:55","2022-01-31T23:59:35","Observation","Ship Staff","Ship Staff Insp.","High seachest Copper anode found not operational","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","RO Raised. communication in progress with office regarding troubleshooting. Spares have been ordered. Once received it will be installed and troubleshoot again. Vsl has just completed the part of troubleshooting. Now awaiting new anodes. On office advise, anodes must be replaced on receipt. Same will be replaced and rectified on receipt of the spare.\n New anode received and renewed. System operational\n","2022-06-27T23:59:35","STAI220064","Completed","2022-05-17T23:59:35","No","No","No","Internal"]
[null,null,null,23968,null,"48_08-Feb-22 10:02:35","2022-02-01T23:59:35","Observation","Ship Staff","Ship Staff Insp.","#1 Fuel pump Top cover O rings leaking when LSMGO inuse","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Fuel pump replaced with overhauled spare.","2022-03-22T23:59:35","","Completed","2022-04-04T23:59:35","No","No","No","Internal"]
[null,null,null,23970,null,"48_20-Feb-22 18:21:09","2022-02-02T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Permanent power arrangement for Ben merry in officer’s mess room. Presently it is connected with extension.","Accommodation","Safety / LSA / FFA","Equipment Related,Inappropriate Procedure","","","","","Proper routing will be carried out. Same will be carried out after sailing load port. Cable will be re-routed via proper channel. New fixture is in place to avoid loose cable hangings. Job was completed satisfactorily. same to be closed out.","2022-05-02T23:59:35","","Completed","2022-02-19T23:59:35","No","No","No","Internal"]
[null,null,null,23971,null,"48_20-Feb-22 18:27:28","2022-02-02T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ME FO heater steam inlet valve leaking from gland. To rectify","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Leak will be rectified at suitable oppurtunity.","2022-05-02T23:59:35","","Completed","2022-02-09T23:59:35","No","No","No","Internal"]
[null,null,null,23972,null,"48_20-Feb-22 18:29:32","2022-02-02T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Big sacrificial flanges lying in spare part room unsecured. Permanent securing arrangement to be made.","Miscellaneous","Eng. / Strg. Comp.","Inappropriate Procedure","","","","","Designated place for storage will be provided/ fabricated. Securing arrangements fabrication is in progress in ER Workshop.","2022-05-02T23:59:35","","Completed","2022-03-09T23:59:35","No","No","No","Internal"]
[null,null,null,23973,null,"48_20-Feb-22 18:32:18","2022-02-02T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Lub oil collected in ME fuel pump save all. Leak source to be identified and arrested.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","The oil contained was LSMGO in #4 Fuel pp save all tray. Same is leaking only when changing over to LSMGO and not on HFO. Defect is being reported and repeated in the same list. This one to be close out and main to be followed.The pump is #1 and NOT #4.","2022-05-02T23:59:35","","Completed","2022-02-22T23:59:35","No","No","No","Internal"]
[null,null,null,23974,null,"48_20-Feb-22 18:36:02","2022-02-02T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Port side manifold cargo line drain valve wheel is missing.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","Same will be repaired or replced. Same replaced with spare wheel. Job completed on 15th FEB 2022. Job to be closed out.","2022-05-02T23:59:35","","Completed","2022-02-06T23:59:35","No","No","No","Internal"]
[null,null,null,23975,null,"48_20-Feb-22 18:48:40","2022-02-02T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","IG Deck seal gauge glass to be cleaned as level was not visible.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","Same will be carried out. IG Deck Seal gauge glass cleaning carried out. Job completed on 20th FEB 2022. Job to be closed out.","2022-04-23T23:59:35","","Completed","2022-02-11T23:59:35","No","No","No","Internal"]
[null,null,null,23976,null,"48_20-Feb-22 18:49:55","2022-02-02T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Various hydraulic boxes on deck to derust and paint","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","JOB GOT REPEATED DURING TYPING. SAME IS MADE COMPLETED AND REMOVED FROM MAINSHEET.","2022-05-02T23:59:35","","Completed","2022-02-16T23:59:35","No","No","No","Internal"]
[null,null,null,23977,null,"48_20-Feb-22 18:51:27","2022-02-02T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Cargo tank and ballast tank domes to derust and paint","Cargo Mach.,Miscellaneous","Cargo / Ballast Systems","Equipment Related","8.21","High","","","Same will be carried out. Job is in progress as of 25th FEB 2022.\nCargo tank and ballast tank domes derust and painting completed.","2022-05-02T23:59:35","","Completed","2022-04-02T23:59:35","No","No","No","Internal"]
[null,null,null,23978,null,"48_20-Feb-22 18:46:07","2022-02-02T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ME OMD various alarm LED were appearing and disappearing. To be checked.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","ME OMD was attended on departure SIngapore. Old PCB card was used in ECR panel and #9 unit detector head was replaced with new spare. Vsl monitored for 5 days and reported to office end about running well. Same was discussed with office to continue with old PCB card and not use New PCB card. Both office and Vsl came to an aggreement to continue like this and end testing with new PCB card as it is not working at all. Kindly follow MSG dated 17 FEB 2022/ DHT TAIGA Main Engine Oil Mist Detector (OMD) for reference on orders.","2022-05-02T23:59:35","","Completed","2022-02-08T23:59:35","No","No","No","Internal"]
[null,null,null,23969,null,"48_12/02/2022 7:01:23 PM","2022-02-03T23:59:35","Defect","Others (Eg. Insurance etc.)","","Embarcation ladder Cruddle corroded","Accommodation","Safety / LSA / FFA","External Factors","5.29","High","","","new cruddle to be fabricated. Same in progress of fabrication as of 25th FEB 2022. Port side lifeboat railing cruddle for embarcation ladder replaced with newly fabricted in ER workshop satisfactorily. Job completed. Same to be closed out.","2022-03-01T23:59:35","","Completed","2022-02-17T23:59:35","No","No","No","External"]
[null,null,null,29183,73576,"48_Sun Mar 12 2023 15:09:28 GMT+0800","2022-02-04T23:59:35","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Most of the Bridge officer’s not aware of turning circle.","Navigation - Others","Navigation","Behaviour Based,Knowledge Based","4.20","Very High","","","Required Training carried out by Master for all Deck Officers","2022-05-03T23:59:35","","Completed","2022-02-05T23:59:35","No","No","No","Internal","Please discuss this observation and preventive action in next safety meeting/tool box meeting, with the officers/crew involved, to avoid recurrence."]
[null,null,null,24951,null,"48_29-Mar-22 15:59:27","2022-03-13T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Main engine Servo oil backwash filter solenoid valve malfunctioning. ","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Solenoid valve to be replaced.","2022-03-13T23:59:35","","Completed","2022-03-13T23:59:35","No","No","No","Internal"]
[null,null,null,26924,21692,"48_Tue Sep 20 2022 21:53:30 GMT+0800","2022-05-25T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Main Engine FO auto back flushing filter - Change over spindle leaking .","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","C/O spindle O rings need to be renewed.\nSpindle O rings renewed","2022-07-25T23:59:35","","Completed","2022-06-10T23:59:35","No","No","No","Internal"]
[null,null,null,26925,88999,"48_Tue Sep 20 2022 22:16:59 GMT+0800","2022-05-28T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Aux. Engine - Fuel oil Auto back flushing filter change over spidle leaking from O rings ","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","O rings need to be renewed.\nChange over spindle overhauled, O rings renewed.","2022-07-28T23:59:35","","Completed","2022-06-12T23:59:35","No","No","No","Internal"]
[null,null,null,26928,96891,"48_Wed Sep 21 2022 23:27:07 GMT+0800","2022-06-06T23:59:35","Defect","Ship Staff","Ship Staff Insp.","TG condenser level switch inoperational","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","",""," Need to renew the displacer.Requisition raised for the same.\nSpare received and renewed, system operational","2022-08-05T23:59:35","STAI20038","Completed","2022-07-12T23:59:35","No","No","No","Internal"]
[null,null,null,26936,45750,"48_Wed Sep 21 2022 23:17:35 GMT+0800","2022-06-06T23:59:35","Defect","Ship Staff","Ship Staff Insp.","EGCS over board line de-gasing  valve malfunctioing","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Needs to inspect valve and actuator for proper functioning.\nChecked and made operational","2022-08-15T23:59:35","","Completed","2022-06-26T23:59:35","No","No","No","Internal"]
[null,null,null,26926,87395,"48_Tue Sep 20 2022 22:28:56 GMT+0800","2022-06-10T23:59:35","Defect","Ship Staff","Ship Staff Insp.","HP circulating pump No.1 - Discharge valve passing.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.3","Medium","","","Valve needs to be renewed.\nDischarge valve renewed and tested, working satisfactory","2022-08-12T23:59:35","","Completed","2022-06-16T23:59:35","No","No","No","Internal"]
[null,null,null,26927,60525,"48_Tue Sep 20 2022 22:22:53 GMT+0800","2022-06-10T23:59:35","Defect","Ship Staff","Ship Staff Insp.","LT Cooler - No.2 : Sacrificial flange befor SW outlet valve leaking from the tell tale hole.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","External Factors","","","","","Sacrificial flange need to be renewed.\nSacrificial flange, gaskets and bonding wire renewed.","2022-07-09T23:59:35","","Completed","2022-06-16T23:59:35","No","No","No","Internal"]
[null,null,null,26929,30523,"48_Wed Sep 21 2022 23:45:14 GMT+0800","2022-07-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Fwd Air Whistle  tripping on overload","Navigation - Others","Navigation","Equipment Related","","","","","FWD whislte - reported failure while operation, same checked found the piston is not moving. Removed  air whistle along with motor to workshop. Upon dismantling found crank bearing is broken and stuck. Renewed crank bearing and assembled the unit. Whistle tried out and found working satisfactory.","2022-09-30T23:59:35","","Completed","2022-07-02T23:59:35","No","No","No","Internal"]
[null,null,null,26930,85633,"48_Wed Sep 21 2022 23:56:36 GMT+0800","2022-07-04T23:59:35","Defect","Ship Staff","Ship Staff Insp.","DG2 Pre-lubrication pump seal leaking","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Pump and motor overhauled..Boxed back in place with new seal and bearings.\nTested and found working satisfactory","2022-07-08T23:59:35","","Completed","2022-07-04T23:59:35","No","No","No","Internal"]
[null,null,null,26931,91166,"48_Thu Sep 22 2022 00:07:43 GMT+0800","2022-07-05T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Main engine L.O.and Servo oil auto back wash filter frequently flushing","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Further investigation indicated defect with the fuel injector in which spindle guide complete with nozzle locating pin broken.This  caused the fuel injector spray pattern towards the wall side of the combustion chamber,hence,incomplete combustion. Unburned FO / waxy sludgewas passing through stuffing box to the crank case. the Fuel injector replaced with the spare one and problem got resolved.","2022-07-17T23:59:35","","Completed","2022-07-13T23:59:35","No","No","No","Internal"]
[null,null,null,26932,95943,"48_Thu Sep 22 2022 00:09:45 GMT+0800","2022-07-12T23:59:35","Defect","Ship Staff","Ship Staff Insp.","MELO auto back flushing filter Operating Air  - Pressure reducing valve  leaking due to cracked filter chamber glass, ","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Air Pressure regulating valve - Filter  chamber glass renewed","2022-07-14T23:59:35","","Completed","2022-07-12T23:59:35","No","No","No","Internal"]
[null,null,null,29181,49805,"48_Sun Mar 12 2023 15:02:12 GMT+0800","2022-07-22T23:59:35","Observation","Ship Staff","Nav Audit / Verification","There was no evidence that Leading lights/Transit bearings were used to monitor vessels position while transiting in coastal waters.","Navigation - Others","Navigation","Behaviour Based,Knowledge Based","4.20","Very High","","","Transit Bearings were identified on the route and marked on ECDIS. Transit bearing taken at next available opportunity.","2022-10-25T23:59:35","None","Completed","2022-10-24T23:59:35","No","No","No","Internal","Please discuss this observation and preventive action in next safety meeting/tool box meeting, with the officers/crew involved, to avoid recurrence."]
[null,null,null,26933,90174,"48_Thu Sep 22 2022 00:22:25 GMT+0800","2022-07-24T23:59:35","Defect","Ship Staff","Ship Staff Insp.","4 Nos. of Hydrualic jacks for Main Engine cylinder cover found leaking while testing","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","All of them overhauled. Back up rings and O rings renewed. Hydraulic jacks tested and found satisfactory.","2022-07-30T23:59:35","","Completed","2022-08-26T23:59:35","No","No","No","Internal"]
[null,null,null,26934,11636,"48_Thu Sep 22 2022 02:43:55 GMT+0800","2022-08-02T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Aux. Boiler No.1 - Air servo error during pre purging operation","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","Servo piston found unable to close during pre purge. \nElectro pneumatic contorller valve block renewed. \nPiston degreased, cleaned and oil applied. Boiler tried out and found working satisfactory.","2022-08-09T23:59:35","","Completed","2022-08-04T23:59:35","No","No","No","Internal"]
[null,null,null,26935,67995,"48_Thu Sep 22 2022 03:09:00 GMT+0800","2022-08-05T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Aux. Engine Turbo charger water washing line leakage due to corroded pipe\n","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Branch pipe renewed. ","2022-08-06T23:59:35","","Completed","2022-08-05T23:59:35","No","No","No","Internal"]
[null,null,null,26943,91407,"48_Thu Sep 22 2022 03:10:55 GMT+0800","2022-08-07T23:59:35","Defect","Ship Staff","Ship Staff Insp.","WHRS  Super heater main steam valve - Steam leakage from valve bonnet. ","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Steam leakage from valve bonnet  rectfied by renewing gasket. ","2022-08-07T23:59:35","","Completed","2022-08-07T23:59:35","No","No","No","Internal"]
[null,null,null,26937,68513,"48_Thu Sep 22 2022 03:12:24 GMT+0800","2022-08-11T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Aux. Boiler No.2  Main steam stop valve - Steam leakage from bonnet.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","Steam leakage from bonnet rectified by renewing gasket.","2022-08-11T23:59:35","","Completed","2022-08-11T23:59:35","No","No","No","Internal"]
[null,null,null,26938,49044,"48_Thu Sep 22 2022 03:26:25 GMT+0800","2022-08-14T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Turbine Generator - Sump vent  getting pressurised.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","Oil mist chamber for DGs and TG are common. Oil mist chamber opened and checked for any blockage, found no abnormalities.  Common vent line outlet hood on funnel top dismantled and found the mesh in chocked condition, same cleaned and system back to normal.","2022-08-20T23:59:35","","Completed","2022-08-15T23:59:35","No","No","No","Internal"]
[null,null,null,26939,95898,"48_Thu Sep 22 2022 03:28:03 GMT+0800","2022-08-16T23:59:35","Defect","Ship Staff","Ship Staff Insp.","IG- Deck seal sea water pump discharge pressure low","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","","","","","Both pumps inspected, found impeller eyes blocked.\nOverhauling of both pumps carried out. Anode plates renewed. Pumps tried out and found working satisfactory with 4.5 bar discharge pressure in ballast condition.","2022-08-17T23:59:35","","Completed","2022-08-17T23:59:35","No","No","No","Internal"]
[null,null,null,26940,40898,"48_Thu Sep 22 2022 03:35:23 GMT+0800","2022-08-18T23:59:35","Defect","Ship Staff","Ship Staff Insp.","COPT/Main CSW pump No.3 - leakage through shaft seal","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","","","","","Pump isolated and opened for inspection, found mechancial seal's stationary part broken. Pump overhauling carried out and put in use, found working satisfctory","2022-08-20T23:59:35","","Completed","2022-08-19T23:59:35","No","No","No","Internal"]
[null,null,null,26941,30450,"48_Thu Sep 22 2022 04:05:23 GMT+0800","2022-08-25T23:59:35","Defect","Ship Staff","Ship Staff Insp.","No.1 Aux Boiler Gauge glass (Port side) leaking                                                                                                                                                        ","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","No.1 Aux Boiler Gauge glass (Port side) - Overhauling carried out.- Gakets and glasses renewed.","2022-08-30T23:59:35","","Completed","2022-08-26T23:59:35","No","No","No","Internal"]
[null,null,null,26942,19569,"48_Thu Sep 22 2022 04:22:25 GMT+0800","2022-08-28T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Aux DG - TC inlet A temperature high","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Troubleshooting to carry out.\nAux DG - TC inlet A temperature high trouble shooting carried out. Cartridge opened and inspected. Found TC inlet A line with carbon deposits. Peak pressure of No.3 found lesser . (Unit 2,3 & 5connected to TC  Inlet A line). All units fuel injectors tested and found with in limit.\n TC inlet A manifold  removed,  Unit 3 Exhaust outlet found with unburned deposits. Sealing test done for the same and found exhaust valve leaking. Removed Cylinder head and found hole  on one of the exhaust valve spindle edge. Cylinder head replaced with overhauled one. DG tested on load and found satisfactory.\n","2022-09-04T23:59:35","","Completed","2022-09-01T23:59:35","No","No","No","Internal"]
[null,null,null,26923,15904,"48_Thu Sep 22 2022 04:34:27 GMT+0800","2022-09-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Echo sounder remote display indicator defective","Navigation - Echo Sounder / Speed Log","Navigation","Equipment Related","","","","","Completed","2022-11-30T23:59:35","STAI220194","Completed","2022-11-30T23:59:35","No","No","No","Internal","spares will be arranged and job to be completed on priority"]
[null,null,null,26921,63819,"48_Thu Sep 22 2022 05:58:40 GMT+0800","2022-09-02T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Main steam valve HP super heater  - Malfunctioning.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Checked and overhauled in DD","2022-12-01T23:59:35","","Completed","2022-12-01T23:59:35","No","No","No","Internal","Raise RO and include in DDRL, try to complete during the upcoming docking in Nov 22"]
[null,null,null,26922,16078,"48_Thu Sep 22 2022 05:48:24 GMT+0800","2022-09-02T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Main engine scavenge smoothening main steam valve - pin hole on the valve body","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","New valve received and fitted in DD","2022-12-01T23:59:35","STAI220110","Completed","2022-11-29T23:59:35","No","No","No","Internal","complete the job as planned once the spare valve is received"]
[null,null,null,26944,22371,"48_Thu Sep 22 2022 06:02:10 GMT+0800","2022-09-10T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Main engine Aux. Blower No.,2 - Starter panel contactor malfunctioning","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","MAIN ENGINE AUX.BLOWER AFT: On investigation found that Main contactors 88-1 and 42-1 not energizing fully due to weak magnetic coil causes motor not getting rated voltage. Replaced the magnetic contactors with spare onboard. Carried out simulation test prior starting the blower fan. Circuit found operational. Blower fan tried out and found working satisfactory","2022-09-11T23:59:35","","Completed","2022-09-11T23:59:35","No","No","No","Internal"]
[null,null,null,29188,62661,"48_Mon Mar 13 2023 02:29:44 GMT+0800","2022-10-04T23:59:35","Other,Defect","Ship Staff","Ship Staff Insp.","AIS jog dial was not functioning properly and not moving smoothly when rotating the jog dial.","Navigation - Others","Navigation","Equipment Related","4.2","Medium","","","AIS main control unit was changed at Shekou dry dock due to jog dial was not functioning properly and not moving smoothly when rotating the jog dial. Programming carried out by shore technician and tested the AIS and found working satisfactory.","2022-12-04T23:59:35","None","Completed","2022-11-24T23:59:35","Yes","No","No","Internal","None"]
[null,null,null,29191,45476,"48_Mon Mar 13 2023 03:37:09 GMT+0800","2022-10-04T23:59:35","Other","Ship Staff","Ship Staff Insp.","magnetic compass inspection.","Navigation - Others","Navigation","Equipment Related","4.7","High","","","Shore technician carried out magnetic compass inspection, adjusted and calibrated the magnetic compass at Shekou dry dock .Magnetic compass is working in good condition. Technician issued the deviation table to ship.","2022-12-04T23:59:35","None","Completed","2022-11-29T23:59:35","Yes","No","No","Internal","None"]
[null,null,null,29193,10007,"48_Mon Mar 13 2023 02:23:06 GMT+0800","2022-10-04T23:59:35","Other","Ship Staff","Ship Staff Insp.","Echo sounder annual inspection and installation of forward Transducer.","Navigation - Echo Sounder / Speed Log","Navigation","Equipment Related","4.7","High","","","Shore technician installed new transducer forward (JFE-680) and replaced the old one at dry dock.After installation of new transducer forward, technician together with ship staff and shipyard personnel carried out vacuum test of the same, found Transducer is intact and found system is working satisfactory.","2022-12-04T23:59:35","None","Completed","2022-11-28T23:59:35","Yes","No","No","Internal","None"]
[null,null,null,28442,null,"48_16/01/2023 22:47:36","2022-11-02T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Few Lights found not working/fused in the EGCS control panel platform","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","11.9","Low","","","Fused tube lights renewed","2022-12-09T23:59:35","","Completed","2022-12-04T23:59:35","No","No","No","Internal"]
[null,null,null,29182,35819,"48_Sun Mar 12 2023 15:05:17 GMT+0800","2022-11-02T23:59:35","Observation","Ship Staff","Nav Audit / Verification","Change of watch level was not mentioned in bell book, although it was enterd in deck log book.","Navigation - Others","Navigation","Behaviour Based,Knowledge Based","4.20","Very High","","","All old records were checked and ensured no information is missing from the log books.","2023-01-17T23:59:35","None","Completed","2022-11-02T23:59:35","No","No","No","Internal","Please discuss this observation and preventive action in next safety meeting/tool box meeting, with the officers/crew involved, to avoid recurrence."]
[null,null,null,29187,90195,"48_Sun Mar 12 2023 15:56:40 GMT+0800","2022-11-04T23:59:35","Other","Ship Staff","Ship Staff Insp.","Radar (X&S Band) annual inspection and maintenance due at dry dock","Navigation - RADAR","Navigation","Equipment Related","4.7","High","","","Radar (X&S Band) annual inspection and maintenance was carried out by shore technician at Shekou dry dock.\nBoth radars are installed with new radar magnetron and scanner motor. System checked and found working satisfactory. \n","2023-01-04T23:59:35","","Completed","2022-11-24T23:59:35","Yes","No","No","Internal","None"]
[null,null,null,29192,41082,"48_Mon Mar 13 2023 03:41:16 GMT+0800","2022-11-07T23:59:35","Other","Ship Staff","Ship Staff Insp.","Annual servicing and maintenance of Autopilot.","Navigation - Others","Navigation","Equipment Related","4.7","High","","","Annual servicing and maintenance of Autopilot carried out by shore technician at Singapore. Replaced system selection switch, mode selection switch, linear svnchro motor and buffer PWB. \nSystem checked and tested the unit, and found auto pilot working in good condition.\n","2023-01-07T23:59:35","None","Completed","2022-12-07T23:59:35","No","No","No","Internal","None"]
[null,null,null,29194,18204,"48_Mon Mar 13 2023 03:46:12 GMT+0800","2022-11-07T23:59:35","Other","Ship Staff","Ship Staff Insp.","Annual servicing and maintenance of Gyro Compass No.1 & 2 ","Navigation - Others","Navigation","Equipment Related","4.7","High","","","Annual servicing and maintenance of Gyro Compass No.1 & 2 carried out by shore technician and sensitive element for both Gyro compass changed at Singapore","2023-01-07T23:59:35","None","Completed","2022-12-07T23:59:35","No","No","No","Internal","None"]
[null,null,null,29195,67716,"48_Mon Mar 13 2023 03:49:26 GMT+0800","2022-11-07T23:59:35","Other","Ship Staff","Ship Staff Insp.","VHF System upgrade.","Navigation - GMDSS & Communication","","","4.7","High","","","System upgrade carried out by shore technician at Singapore, all three VHF was updated. System checked and verified found working satisfactory.Trans receiver: 03.22 and Controller: 03.22 \n","2023-01-07T23:59:35","","Completed","2022-12-07T23:59:35","No","No","No","Internal","None"]
[null,null,null,29190,80329,"48_Mon Mar 13 2023 03:02:29 GMT+0800","2022-11-24T23:59:35","Other","Ship Staff","Ship Staff Insp.","ECDIS NO.2 Malfunction display-After installation of new Radar magnetrons and scanner motors, it was found that ECDIS no.2 radar overlay function showing incorrect value.","Navigation - ECDIS","Navigation","Equipment Related","4.7","High","","","Technician checked the CCRP settings and radar settings range and bearing, etc. found it mainly caused by monitor resolution ratio and overlay adjustment. Then technician carried out adjustment refer to the No.1 ECDIS. Now the No.2 ECDIS working normal. System working satisfactory.","2023-02-22T23:59:35","None","Completed","2022-11-24T23:59:35","Yes","No","No","Internal","None"]
[null,null,null,28434,null,"48_16-Jan-23 11:40:49","2022-12-02T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Port & Stbd midship locker found not arranged and items not secured","Miscellaneous","ISM Related","Industry Issue","11.3","Medium","","","Both midship lkr squared up, items secured, floor cleaned","2022-12-17T23:59:35","","Completed","2022-12-12T23:59:35","No","No","No","Internal"]
[null,null,null,28435,null,"48_16-Jan-23 11:52:22","2022-12-02T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Found inboard side retro reflective tape on Port side life boat also painted during DD maintenance / painting job, same need to be renewed with new one. ","LSA / FFA","Safety / LSA / FFA","Inappropriate Procedure","5.27","Medium","","","Retro reflective tapes renewed in port side inboard side, no more in the bad condition.","2022-12-09T23:59:35","","Completed","2022-12-06T23:59:35","No","No","No","Internal"]
[null,null,null,28436,null,"48_16-Jan-23 12:00:04","2022-12-02T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","One of the wire sling found without SWL tag inside port side midship locker, same need to be discarded. ","Cargo Mach.,Miscellaneous","ISM Related","Equipment Related,Industry Issue","10.28","Low","","","Item immediately removed and discarded. put discarded tag and kept in garbage room for landing. ","2022-12-02T23:59:35","","Completed","2022-12-02T23:59:35","No","No","No","Internal"]
[null,null,null,28437,null,"48_16-Jan-23 12:03:24","2022-12-02T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Ship’s accommodation ladders were load tested in dry dock. load test date stenciling found missing on the P & S side ladder. ","Deck - Machinery","ISM Related","Human Error,Industry Issue","5.47","Medium","","","Stencilling done in both side ladder.","2022-12-09T23:59:35","","Completed","2022-12-06T23:59:35","No","No","No","Internal"]
[null,null,null,28438,null,"48_16-Jan-23 12:11:15","2022-12-02T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Pump room entry procedure at entrance faded and same need to be replaced. ","Miscellaneous","Cargo / Ballast Systems","External Factors","8.29","High","","","Pump room entry  procedure pasted / renewed ","2022-12-09T23:59:35","","Completed","2022-12-03T23:59:35","No","No","No","Internal"]
[null,null,null,28439,null,"48_16/01/2023 22:40:13","2022-12-02T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","#1 Boiler safety valve flange is not covered with lagging","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","#1 Boiler safety valve flange covered with lagging","2022-12-09T23:59:35","","Completed","2022-12-05T23:59:35","No","No","No","Internal"]
[null,null,null,28440,null,"48_16/01/2023 22:44:02","2022-12-02T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","HP drum feed water valve leaking from gland, to repair","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Gland renewed and leak rectified","2022-12-17T23:59:35","","Completed","2022-12-08T23:59:35","No","No","No","Internal"]
[null,null,null,28444,null,"48_16/01/2023 22:55:01","2022-12-02T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","DG Exhaust pipe seal pot not having water. To top up water and maintain.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Seal pot filled with water below overflow level","2022-12-09T23:59:35","","Completed","2022-12-08T23:59:35","No","No","No","Internal"]
[null,null,null,28601,49022,"48_Wed Feb 01 2023 18:24:02 GMT+0800","2022-12-02T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Found inboard side retro reflective tape on Port side life boat also painted during DD maintenance / painting job, same need to be renewed with new one. ","LSA / FFA","Safety / LSA / FFA","Inappropriate Procedure","5.27","Medium","","","Retro reflective tapes renewed in port side inboard side, no more in the bad condition.\n","2022-12-09T23:59:35","","Completed","2022-12-06T23:59:35","No","No","No","Internal"]
[null,null,null,28602,22762,"48_Wed Feb 01 2023 18:28:35 GMT+0800","2022-12-02T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","One of the wire sling found without SWL tag inside port side midship locker, same need to be discarded. ","Cargo Mach.,Miscellaneous","ISM Related","Equipment Related,Industry Issue","10.28","Low","","","Item immediately removed and discarded. put discarded tag and kept in garbage room for landing. \n","2022-12-02T23:59:35","","Completed","2022-12-02T23:59:35","No","No","No","Internal"]
[null,null,null,28603,15115,"48_Wed Feb 01 2023 18:35:10 GMT+0800","2022-12-02T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Pump room entry procedure at entrance faded and same need to be replaced. \n","Miscellaneous","Cargo / Ballast Systems","External Factors","8.29","High","","","Pump room entry  procedure pasted / renewed \n","2022-12-09T23:59:35","","Completed","2022-12-03T23:59:35","No","No","No","Internal"]
[null,null,null,28604,11801,"0_Wed Feb 01 2023 18:39:03 GMT+0800","2022-12-02T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Some of the ballast tank vent flame screen found damaged","Deck - Machinery","Cargo / Ballast Systems","Industry Issue,External Factors","11.7","High","","","Rusted vent screen renewed in places","2022-12-17T23:59:35","","Completed","2022-12-13T23:59:35","No","No","No","Internal"]
[null,null,null,28605,89391,"48_Wed Feb 01 2023 18:32:11 GMT+0800","2022-12-02T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Ship’s accommodation ladders were load tested in dry dock. load test date stenciling found missing on the P & S side ladder. ","Deck - Machinery","ISM Related","Human Error","5.47","Medium","","","Stenciling done in both side ladder.\n","2022-12-09T23:59:35","","Completed","2022-12-06T23:59:35","No","No","No","Internal"]
[null,null,null,28606,80523,"48_Wed Feb 01 2023 19:03:01 GMT+0800","2022-12-02T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","#1 Boiler safety valve flange is not covered with lagging","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","#1 Boiler safety valve flange covered with lagging","2022-12-09T23:59:35","","Completed","2022-12-05T23:59:35","No","No","No","Internal"]
[null,null,null,28607,91975,"48_Wed Feb 01 2023 19:06:37 GMT+0800","2022-12-02T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","HP drum feed water valve leaking from gland to repair","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Gland renewed and leak rectified","2022-12-17T23:59:35","","Completed","2022-12-08T23:59:35","No","No","No","Internal"]
[null,null,null,28608,79018,"48_Wed Feb 01 2023 19:10:12 GMT+0800","2022-12-02T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","DG exhaust pipe seal pot not having water. To top up water and maintain","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Seal pot filled with water below overflow level","2022-12-09T23:59:35","","Completed","2022-12-08T23:59:35","No","No","No","Internal"]
[null,null,null,28614,60401,"48_Wed Feb 01 2023 18:19:44 GMT+0800","2022-12-02T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Port & Stbd midship locker found not arranged and items not secured. ","Miscellaneous","General Appearance","Industry Issue","11.3","Medium","","","Both midship lkr squared up, items secured, floor cleaned\n","2022-12-17T23:59:35","","Completed","2022-12-12T23:59:35","No","No","No","Internal"]
[null,null,null,29179,98336,"48_Sun Mar 12 2023 14:38:11 GMT+0800","2022-12-07T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","Doppler log was operational and was working good till vessel arrived dry dock. Old transducer, its socket and cable were in good working condition when it was opened for replacement at dry dock. Technicians renewed the doppler log transduer at dry dock but it was observed that doppler log is not showing correct reading on display unit on the bridge. ","Navigation - Echo Sounder / Speed Log","Navigation","Equipment Related","4.7","High","","","JRC Techinician attended at singapore call and they found that the transducer socket damaged and burnt out due to sort circuit. Master advise to replace the faulty Transducer and wire to  new Transducer,  Technician together with ships crew installed new transducer and wire for the same. Syestem checked found working satisfactory . No erractic readings.\n\n","2023-02-19T23:59:35","None","Completed","2023-01-19T23:59:35","No","No","No","Internal","None"]
[null,null,null,29180,10091,"48_Sun Mar 12 2023 14:51:22 GMT+0800","2022-12-07T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","DC Dimmer switch for magnetic compass was not operational.","Navigation - Others","Navigation","Equipment Related","4.7","High","",""," DC Dimmer bulb changed for magnetic compass and tested , all found working condition","2023-01-06T23:59:35","None","Completed","2022-12-08T23:59:35","No","No","No","Internal"]
[null,null,null,29184,40103,"48_Sun Mar 12 2023 15:22:30 GMT+0800","2022-12-08T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Ecdis 1 & 2  processing unit hard disck batteies  found expired. but system found to be working satisfactory. ","Navigation - ECDIS","Navigation","Equipment Related","4.7","High","","","Ecdis 1 & 2 processing unit Hard disk batteries replaced with new one. System checked and found working satisfactory.","2023-03-08T23:59:35","None","Completed","2023-02-03T23:59:35","No","No","No","Internal","None"]
[null,null,null,29185,73884,"48_Sun Mar 12 2023 15:33:58 GMT+0800","2022-12-08T23:59:35","Other","Ship Staff","Ship Staff Insp.","No.1 & 2 ECDIS annual Complete health checks on hardware.\nChecks on internal batteries and Checks on track ball, Keyboard and associate cooling fans.Checks on present software and upgrade it if necessary as per IHO and PL.4.0.Latest upgrade to software was due shore servicing.\n","","Navigation","Behaviour Based","4.7","High","","","Annual servicing carried out by JRC technician and system checked and found working satisfactory.","2023-02-03T23:59:35","None","Completed","2023-01-19T23:59:35","No","No","No","Internal","None"]
[null,null,null,29186,45183,"48_Sun Mar 12 2023 15:49:18 GMT+0800","2022-12-08T23:59:35","Other","Ship Staff","Ship Staff Insp.","NAV 1&2 Laptops was found no Back up power supply and no UPS fitted to feed power in case of AC supply is not available.","Navigation - Others","Navigation","Equipment Related","4.1","High","","","Vessel has new UPS and same has been installed for Both Nav & 2 Laptops. Checked both Laptops by removing the Ac supply, found unintrupted power to Laptops through UPS. 2 UPS are intalled to have independent power supply","2023-02-08T23:59:35","None","Completed","2022-12-31T23:59:35","No","No","No","Internal","None"]
[null,null,null,28433,null,"48_16/01/2023 21:27:50","2022-12-08T23:59:35","Defect","Ship Staff","Ship Staff Insp.","ME Flowmeter not showing any reading after technician attendance for Kyma and Flowmeter sync","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","ME flowmeter PCB replaced by Emerson technician and made operational. Kyma remote trouble shooting done and sync with ME flowmeter established.","2023-02-07T23:59:35","PO issued from office","Completed","2023-01-23T23:59:35","No","No","No","Internal","Serv arranged in Singapore again on 26th Jan,"]
[null,null,null,28612,73402,"48_Wed Feb 01 2023 19:25:33 GMT+0800","2022-12-08T23:59:35","Defect","Ship Staff","Ship Staff Insp.","ME flowmeter not showing any reading after technician attendance for KYMA and flowmeter sync","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","ME flowmeter PCB replaced by Emerson technician and made operational. Kyma remote trouble shooting done and sync with ME flowmeter established.","2023-02-07T23:59:35","","Completed","2023-01-23T23:59:35","No","No","No","Internal","The issue is already in discussion with Emerson and KYMA.  Emerson promised to solve the issue at earliest.  KYMA mentions data is not being received however system seems ok. "]
[null,null,null,28610,27669,"48_Wed Feb 01 2023 19:32:55 GMT+0800","2022-12-12T23:59:35","Defect","Ship Staff","Ship Staff Insp.","#2 ME LO pump not providing sufficient discharge pressure after overhaul in DD. Suspect blockage in the bellow.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","#2 ME LO pump lifted up and checked for clogging., found none. LO sump emptied and found left over rags from DD. Same removed and fault rectified.","2023-02-12T23:59:35","","Completed","2023-01-17T23:59:35","No","No","No","Internal"]
[null,null,null,28598,46874,"48_Wed Feb 01 2023 19:21:26 GMT+0800","2022-12-26T23:59:35","Defect","Ship Staff","Ship Staff Insp.","#1 HFO purifier 3/2 way valve leaking from shaft seal","E/R - Purifier","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Leaking shaft seal sealing rings and gasket replaced and leak rectified","2023-03-25T23:59:35","","Completed","2023-01-27T23:59:35","No","No","No","Internal","Will arrange spare but meanwhile pls open and overhaul to see if can be repaired by onboard consumable spares."]
[null,null,null,28441,null,"48_16/01/2023 21:37:57","2022-12-27T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Forward horn found not working","Navigation - Others","Navigation","Equipment Related","12.12","High","","","Horn opened up and found bearing hard to turn. Same replaced with new bearing and piston and rings cleaned and boxed back. Tested horn and found working good","2023-01-03T23:59:35","","Completed","2023-01-01T23:59:35","No","No","No","Internal"]
[null,null,null,28443,null,"48_16/01/2023 21:45:49","2022-12-27T23:59:35","Defect","Ship Staff","Ship Staff Insp.","AUx DG exhaust bellow at incinerator platform found leaking","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.19","Very High","","","Bellow replaced with new spare bellow and leak rectified.","2023-01-03T23:59:35","","Completed","2022-12-29T23:59:35","No","No","No","Internal"]
[null,null,null,28609,47421,"48_Wed Feb 01 2023 19:14:09 GMT+0800","2022-12-27T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Foward horn found not working","Navigation - RADAR,Navigation - Others","Navigation","Equipment Related","12.12","High","","","Horn opened up and found hard to turn. Same replaced with new bearing and piston, rings cleaned and boxed back.Tested horn and found working good.","2023-01-03T23:59:35","","Completed","2023-01-01T23:59:35","No","No","No","Internal"]
[null,null,null,28611,19936,"48_Wed Feb 01 2023 19:17:44 GMT+0800","2022-12-27T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Aux DG exhaust bellow at incinerator platform found leaking","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.19","Very High","","","Below replaced with new spare bellow and leak rectified.","2023-01-03T23:59:35","","Completed","2022-12-29T23:59:35","No","No","No","Internal"]
[null,null,null,28613,28978,"48_Wed Jan 18 2023 11:40:59 GMT+0800","2022-12-27T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Aux. DG exhaust Bellow at incinerator platform found leaking.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.19","Very High","","","Bellow replace with new spare bellow and leak  rectified","2023-01-03T23:59:35","","Completed","2022-12-29T23:59:35","No","No","No","Internal"]
[null,null,null,28753,96225,"48_Mon Feb 13 2023 19:42:45 GMT+0800","2023-01-11T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Pump room gas detection system displaying O2 low alarm with -0% O2 reading.","Miscellaneous","Cargo / Ballast Systems","Equipment Related","5.21","Medium","","","Spare received. O2 sensor replaced and calibrated.","2023-04-10T23:59:35","STAI230033\t- PUMP ROOM GAS SAMPLING SYSTEM","Completed","2023-03-09T23:59:35","No","No","No","Internal","Spares to be arrranged for connection on priority. make RA for the same and take additional precautions."]
[null,null,null,28758,25921,"48_Mon Feb 13 2023 19:35:21 GMT+0800","2023-01-15T23:59:35","Observation","Ship Staff","Ship Staff Insp.","VECS O2 sensor not showing correct value even after calibration","Cargo Mach.,Miscellaneous","Cargo / Ballast Systems","Equipment Related","8.17","Low","","","Spare new O2 sensor received and replaced","2023-02-20T23:59:35","STAI230034 - VAPOUR MONITORING SYSTEM","Completed","2023-02-01T23:59:35","No","No","No","Internal"]
[null,null,null,28599,47599,"48_Wed Feb 01 2023 19:54:25 GMT+0800","2023-01-22T23:59:35","Defect","Ship Staff","Ship Staff Insp.","ME FO HP pump leak off tank body cracked and tracing steam leaking","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Leak off tank removed and cracked body welded.","2023-02-07T23:59:35","","Completed","2023-01-26T23:59:35","No","No","No","Internal"]
[null,null,null,28754,15968,"48_Wed Feb 15 2023 18:23:13 GMT+0800","2023-01-24T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","All mooring winch brake linings renewal over due ","Deck - Mooring Machinery","Mooring","Industry Issue,Equipment Related","9.15","Medium","","","RO ( STAI230006) raised for brake lining as the earlier brake lining received were out of spec, New 16 nos brake lining received at last call SGP on 26-Jan-2023, work in progress in FWD brake lining and will be completed soon. All brake linings renewed and winch no 6 & 8 brake lining inspected found in good condition and completed on condition based. ","2023-02-10T23:59:35","","Completed","2023-02-10T23:59:35","No","No","No","Internal"]
[null,null,null,28759,91260,"48_Wed Feb 15 2023 17:58:58 GMT+0800","2023-01-24T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","Stbd side bridge wing flush door for bridge front window unusable due to latch broken while securing / closing ","Miscellaneous","Structural Condn. / WT integrity ","External Factors,Equipment Related","8.40","High","","","The door removed and brought to the E/R workshop for fabrication of the defective latch. Latch fabricated and area de-rusted , painted and put back in place. ","2023-04-23T23:59:35","","Completed","2023-02-06T23:59:35","No","No","No","Internal"]
[null,null,null,28757,15359,"48_Thu Feb 16 2023 03:36:47 GMT+0800","2023-01-28T23:59:35","Defect","Ship Staff","Ship Staff Insp.","LP temperature probe 4 nos out of range.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","LP temperature probe replaced with new spare.","2023-04-26T23:59:35","STAI230044\t- LP TEMPERATURE PROBE- EXHAUST GAS BOILER","Completed","2023-03-12T23:59:35","No","No","No","Internal","spares confirmed for supply , awaiting readiness"]
[null,null,null,28760,32491,"0_Wed Feb 15 2023 18:09:45 GMT+0800","2023-01-28T23:59:35","Defect","Ship Staff","Ship Staff Insp.","There are 2 boxes each near port and stbd side boat deck to keep extra life jacket and immersion suit in the boat deck area for emergency. This metal boxes was corroded and after de-rusting ops, found one of the box cover is cracked, damaged and wasted. Need to carry out fabrication job inside E/R work shop. ","LSA / FFA","ISM Related","Equipment Related","5.27","Medium","","","Damaged box cover was removed and de- rusted thoroughly, same  was taken to E/R for fabrication job. Box cover fabricated and painted and also replaced in its designated place.","2023-04-27T23:59:35","","Completed","2023-02-07T23:59:35","No","No","No","Internal"]
[null,null,null,28755,41923,"48_Thu Feb 16 2023 04:19:56 GMT+0800","2023-01-30T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Spool pipe between Jet sprayer inlet valve and Jet sprayer casing holed.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Spare new pipe fabricated and fitted in place. Leak rectified.","2023-03-12T23:59:35","","Completed","2023-03-03T23:59:35","No","No","No","Internal","complete and close out as planned"]
[null,null,null,28885,92870,"48_Wed Mar 01 2023 00:03:09 GMT+0800","2023-02-02T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","While during de-rusting of fwd ballast tank vents, steel covers of flame screen cracked. As the they were fully rusted and due to low thickness plates completely wasted and cracked.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related,External Factors,Industry Issue","8.1","Very High","","","Items removed and fully chipped and placed in E/R workshop for fabrication job. Item fabricated and re-installed. ","2023-03-01T23:59:35","","Completed","2023-02-23T23:59:35","No","No","No","Internal","complete and close out as planned, raise RO if required"]
[null,null,null,28888,29464,"48_Tue Feb 28 2023 23:49:33 GMT+0800","2023-02-10T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","During deck round found VRCS hyd  return line  for hydraulic valves on deck leaking. Line found rusted heavily and leak is near the pipe bend.","Deck - Machinery","Cargo / Ballast Systems","External Factors,Equipment Related","6.4","High","","","VRCS line and valves going to and from hyd boxes isolated. Notice posted on VRCS pump, not to operate. Line removed and fabricated in E/R work shop. New line and new flange installed. line painted with two coat of primer and re-installed in place. System tried out starting the pump, found no more leakage. ","2023-03-01T23:59:35","","Completed","2023-02-17T23:59:35","No","No","No","Internal"]
[null,null,null,28886,92324,"48_Wed Mar 01 2023 01:37:15 GMT+0800","2023-02-15T23:59:35","Defect","Ship Staff","Ship Staff Insp.","During de-rusting of stbd side life boat deck life jacket box, found box cover metal hinge wasted.","LSA / FFA","Safety / LSA / FFA","External Factors","5.27","Medium","","","One new hinge to be fabricated in E/R work shop and to be installed  with nut bolt assembly . Item fabricated and re-installed in place. ","2023-05-14T23:59:35","","Completed","2023-02-26T23:59:35","No","No","No","Internal","complete and close out as planned"]
[null,null,null,29189,44432,"48_Mon Mar 13 2023 02:57:16 GMT+0800","2023-02-16T23:59:35","Breakdown","Ship Staff","Ship Staff Insp."," DGPS No. 02 display unit was continuously flickering with display unit screen totally blank.","Navigation - DGPS / EPFS / AIS","Navigation","Equipment Related","4.7","High","","","The DGPS No.2 display unit(Serial no-KF48986, Model-NWZ-4740/JLR7800) was switched off and antenna connections were checked and found all intact.\nDGPS was re-started after 10 minutes but display unit was still flickering with screen totally blank.\nVessel has two spare DGPS display units – one brand new (Serial no-KG13134, Model-NWZ-4740), other used unit but marked as in working condition(Serial no-KF11840, Model-NWZ-4740/JLR7500).\n\nWe replaced the DGPS No.2 display unit with old spare display unit(Serial no-KF11840, Model-NWZ-4740/ JLR7500) and found to be working good after doing initial initialization and setup. All the parameters checked / compared with DGPS No.1 and found all in order.\nDGPS No.2 display unit is under observation and being continuously monitored by duty officers and working satisfactory.\n","2023-05-16T23:59:35","None","Completed","2023-02-16T23:59:35","No","No","No","Internal","None"]
[null,null,null,28887,15763,"48_Wed Mar 01 2023 01:29:02 GMT+0800","2023-02-17T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Stbd side Hose handling crane personal transfer operating wire lever found broken.","Deck - Machinery","ISM Related","Equipment Related","8.63","High","","","New lever to be fabricated and reinstalled before arrival load port. Installed new lever, now working satisfactory. ","2023-03-01T23:59:35","","Completed","2023-02-26T23:59:35","No","No","No","Internal","complete and close out as planned"]
[null,null,null,28889,43731,"48_Wed Mar 01 2023 01:50:52 GMT+0800","2023-02-19T23:59:35","Observation","Ship Staff","Ship Staff Insp.","After opening no 1 BWTS back wash filter for cleaning of candles found 5 candle are missing and one candle is damaged.","Miscellaneous","Cargo / Ballast Systems","Equipment Related,Industry Issue","6.21","High","","","Vessel received 10 candles in last DD, 6 nos of new candles renewed in no 1 BWTS filter unit including damaged one. Old candles cleaned with fresh water removed all rust and reinstalled.","2023-03-22T23:59:35","STAI240074","Completed","2023-02-20T23:59:35","No","No","No","Internal"]
[null,null,null,29177,58950,"48_Wed Mar 15 2023 22:46:03 GMT+0800","2023-03-02T23:59:35","Defect","Ship Staff","Ship Staff Insp.","DG#1 bearing temperature display unit PCB on the engine defective. Bearing temperature can be monitored on AMS monitor in the ECR.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Confirmed PCB defective by replacing from #2 DG. Requisition raised.PCB received while passing Singapore on 28th Singapore replaced and now in working condition.","2023-09-13T23:59:35","STAI230058 - MAIN DG NO 1 LOCAL INSTUMENT PANEL SPARES","Completed","2023-08-30T23:59:35","No","No","No","Internal","complete and close out as planned. \ninitial spares arranged incorrect supply, awaiting exchange and reconnect correct spares."]
[null,null,null,29178,98470,"48_Thu Mar 16 2023 01:01:42 GMT+0800","2023-03-07T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Sewage treatment plant air hose from #2 blower to plant leaking","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Spare hose located and replaced the leaking hose for #2 blower","2023-05-06T23:59:35","","Completed","2023-03-20T23:59:35","No","No","No","Internal","please include the RO number in reference column.\ncomplete and close out as planned."]
[null,null,null,29749,87761,"48_Mon Apr 10 2023 21:26:27 GMT+0800","2023-03-13T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","Internet feed to the Navbox system is not coming and therefore the navstick is not updating through Navbox.","Navigation - Others","Navigation","Equipment Related","4.7","High","","","IT departments and Navtor technical departments informed and followed procedures to check the connections and power cable and found all intact. Techinician advise to chnage the navbox and same has been reported to IT departments. Awaiting new navbox for installation. ECDIS weekly updates is being performed using NAVSYNC and suitability and error in updates is been checked at regular intervals, Both ecdis being updated and working satisfactory.","2023-05-17T23:59:35","None","Completed","2023-04-19T23:59:35","No","No","No","Internal","None"]
[null,null,null,29607,78235,"48_Thu Mar 30 2023 20:00:14 GMT+0800","2023-03-15T23:59:35","Defect","Ship Staff","Ship Staff Insp.","During educting (de-ballasting) operation at Corpus christi with no 2 electric ballast pump in BWTS mode found stbd side ballast eductor line connected with ballast eductor valve  (BA 028) , is unusable, because eductor is not taking suction after opening valve. In spite water going out from the tank , it is observed to be filling. Though the valve is opening / closing freely.  When eductor is put in port side line opening valve no BA 029 then eductor is taking full suction. As the stbd side is connected to stbd tanks and very much required for educting of the stbd side tanks. ","Deck - Pipe / Fittings,Miscellaneous","Cargo / Ballast Systems","External Factors,Equipment Related","8.8","Medium","","","Thorough observation and test  done as follows,\n1) All the valves in the pump room tested for opening closing \nfound all the valves are working remotely except v/v no BA 035 which is a line valve connecting to the stbd line, valve was manually opened from locally. Valve movement checked from ccr and hydraulic room, valve problem rectified, v/v indication prob lem also solved. \n2) All the ballast eductor gauges were also malfuncting, work done, gauge connection removed , air blown through, lots of dirt and accumulated mud drained and gauges stsrted moving. \n3) valve no BA 028 /BA 029 operated and found normal , entered into p/r void space for fault finding but nothing abnormality was found. \n4) After closing all the line valve eductor tried out starting no 2 electric ballast pump. \n5) Both line valve 029 /028 opened one by one and lines sucked found full suction created and eductor running without any prob.\n6) Water sucked from aft tank remaining and found working satisfactory. ","2023-06-15T23:59:35","","Completed","2023-04-04T23:59:35","No","No","No","Internal"]
[null,null,null,28752,87959,"48_Thu Feb 16 2023 03:55:25 GMT+0800","2023-03-17T23:59:35","Defect","Ship Staff","Ship Staff Insp.","BWTS connection terminal for valve (BT-1211) before the backwash filter of #1 system is damaged.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","6.21","High","","","RO raised spares received and fitted in place.","2023-07-27T23:59:35","STAI230046 - BWTS TRO UNIT AND FILTER UNIT VALVE","Completed","2023-07-14T23:59:35","No","No","No","Internal","Spares processed for supply. filter unit valve will not be required in future due to upcoming non filter upgrade expected soon."]
[null,null,null,29603,59260,"48_Sun Apr 02 2023 10:55:46 GMT+0800","2023-03-17T23:59:35","Other","Ship Staff","Ship Staff Insp.","ME fuel pump riser pipe O-ring for all fuel oil pumps to replace at suitable opportunity.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","The riser pipe O ring renewed with new spare O ring , leak rectified.","2023-11-29T23:59:35","STAI230076 received waiting for opportunity to complete.","Completed","2023-10-22T23:59:35","No","No","No","Internal","complete as planned and close out"]
[null,null,null,29605,11923,"48_Sun Apr 02 2023 10:49:27 GMT+0800","2023-03-19T23:59:35","Defect","Ship Staff","Ship Staff Insp.","ME SERVO OIL PUMP FLOW MONITOR #2 FAULTY","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","The Monitor and the sensor renewed with new spare received , now the system is working without any alarms. \n","2023-10-30T23:59:35","STAI230067 - ME SERVO OIL PUMP FLOW SENSOR WITH MONITOR","Completed","2023-10-20T23:59:35","No","No","No","Internal","spares awaiting connection."]
[null,null,null,29604,24981,"48_Sun Apr 02 2023 11:02:40 GMT+0800","2023-03-22T23:59:35","Observation","Ship Staff","Ship Staff Insp.","#2 FWG ejector pump found developing less pressure in loaded passage resulting in developing lower vacuum.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.31","Very High","","","The pump casing repaired with bronze putty and the corrocoat paint applied and after curing the pump boxed with new spare top cover, the shaft , sleeve and the mechanical seal renewed with new spare. The pump tried out , it is found building up pressure, the performance of both the pump and the FWG is found satisfactory. \n","2023-10-29T23:59:35","STAI230210, STAI235042.","Completed","2023-10-03T23:59:35","No","No","No","Internal",""]
[null,null,null,29606,69255,"48_Sun Apr 02 2023 06:21:29 GMT+0800","2023-03-24T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Stbd & port side manifold pressure transmitter box and metal support found wasted in places and need renewal ","Deck - Machinery","Cargo / Ballast Systems","External Factors,Equipment Related","8.41","Medium","","","New boxes procured during DD, and job planned and started during loaded voy.  3 nos of boxes already done, 3 more in progress. \nLast 3 boxes also fabricated and installed in port side manifold to accommodate pressure transmitters. Job completed satisfactory. ","2023-06-23T23:59:35","","Completed",null,"No","No","No","Internal"]
[null,null,null,29940,null,"48_Wed May 10 2023 03:24:36 GMT+0000","2023-04-24T23:59:35","Defect","Ship Staff","Ship Staff Insp.","While taking round in pump room found pump room bottom platform railing small dia pipe is damaged in one place .","Deck - Pipe / Fittings","General Appearance","Knowledge Based","5.17","Very High","","","Cold work carried out","2023-07-23T23:59:35","","Completed","2023-05-17T23:59:35","No","No","No","Internal","Noted hotwork in next DD and cold repair planned in this month."]
[null,null,null,29941,null,"48_Wed May 10 2023 03:27:14 GMT+0000","2023-04-25T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Port side Midship HHC man riding wire renewal is due","Deck - Machinery","Cargo / Ballast Systems","Equipment Related","9.3","Very High","","","Wire Renewed","2023-06-07T23:59:35","2310042","Completed","2023-05-18T23:59:35","No","No","No","Internal","Pls revert with last wire renewal date."]
[null,null,null,30263,86265,"48_Fri Jun 02 2023 21:43:42 GMT+0800","2023-05-15T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Hydroblaster Onboard is In Operational","Miscellaneous","General Appearance","Inappropriate Procedure","","","","","Spares Received, parts fitted in place Hydro blaster tested for its operation found found building up pressure 1050 bar, working satisfactory. ","2023-08-14T23:59:35","","Completed","2023-07-19T23:59:35","No","No","No","Internal","spares processed for supply awaiting connection."]
[null,null,null,30276,12364,"48_Fri Jun 02 2023 21:39:11 GMT+0800","2023-05-15T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Hydraulic leak from Port side windlass Brake cylinder ","Deck - Mooring Machinery","Mooring","Equipment Related","9.20","Medium","","","Oil seal Renewed","2023-06-14T23:59:35","","Completed","2023-05-24T23:59:35","No","No","No","Internal"]
[null,null,null,30278,27155,"48_Sat Jun 03 2023 17:39:39 GMT+0800","2023-05-15T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Compactor is In operational","Miscellaneous","MARPOL Related","Equipment Related","","","","","Renewed the starter panel & electric cable. Working satisfactory","2023-07-14T23:59:35","","Completed","2023-05-25T23:59:35","No","No","No","Internal"]
[null,null,null,30280,23303,"48_Sat Jun 03 2023 20:40:00 GMT+0800","2023-05-16T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Steam Leak from  ME unit #1 Steam Tracing Line Front of ECR","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.12","Very High","",""," Change flange gasket","2023-06-16T23:59:35","","Completed","2023-05-17T23:59:35","No","No","No","Internal"]
[null,null,null,30281,15596,"0_Sat Jun 03 2023 20:46:23 GMT+0800","2023-05-16T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","EGB Casing soft patch  to repair","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.12","Very High","","","Completed Repaired. ","2023-06-16T23:59:35","","Completed","2023-05-20T23:59:35","No","No","No","Internal"]
[null,null,null,30282,55209,"0_Sat Jun 03 2023 20:50:30 GMT+0800","2023-05-16T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","HFO Transfer Pump Gauge to secure with the securing plate","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.12","Very High","","","Job completed pressure gauge secured with  plate.","2023-05-25T23:59:35","","Completed","2023-05-19T23:59:35","No","No","No","Internal"]
[null,null,null,30283,66988,"0_Sat Jun 03 2023 20:55:55 GMT+0800","2023-05-16T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Steering Gear cross head grease  nipples to clean and mark for monthly greasing","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.12","Very High","",""," Cleaned and painted for marking ",null,"","Completed","2023-05-21T23:59:35","No","No","No","Internal"]
[null,null,null,30266,36997,"48_Sat Jun 03 2023 17:01:13 GMT+0800","2023-05-25T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Aft mooring hyd line penetration piece to renew","Deck - Mooring Machinery","General Appearance","Equipment Related","11.4","Very High","",""," Fabricated & renewed the pipe section","2023-06-24T23:59:35","","Completed","2023-06-01T23:59:35","No","No","No","Internal","complete the repairs as planned and close out"]
[null,null,null,30267,83566,"48_Sat Jun 03 2023 17:08:52 GMT+0800","2023-05-25T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Various hydraulic boxes on deck, VECS lines to derust, repair and paint","Deck - Pipe / Fittings","General Appearance","Inappropriate Procedure","11.4","Very High","","","De rusting & painting Of VRCS Hydraulic boxes Completed.","2023-07-24T23:59:35","","Completed","2023-07-18T23:59:35","No","No","No","Internal","complete as planned and close out"]
[null,null,null,30268,78316,"48_Sat Jun 03 2023 17:11:08 GMT+0800","2023-05-25T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","SAAB domes internal cleaning and flange gasket to repair.","Cargo Mach.","Cargo / Ballast Systems","Inappropriate Procedure","","","","","De rusting / painting Completed","2023-06-24T23:59:35","","Completed","2023-06-17T23:59:35","No","No","No","Internal","complete as planned and close out"]
[null,null,null,30269,63225,"48_Sat Jun 03 2023 17:13:22 GMT+0800","2023-05-25T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","EGCS tower ventilation louver on Port side drain line - one section to renew.","Deck - Pipe / Fittings","General Appearance","Inappropriate Procedure","11.4","Very High","","","Fabricated & renewed","2023-06-24T23:59:35","","Completed","2023-06-03T23:59:35","No","No","No","Internal","complete as planned and close out"]
[null,null,null,30270,67310,"48_Sat Jun 03 2023 17:15:35 GMT+0800","2023-05-25T23:59:35","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Deck machinery all the machines, stencil total grease points, high light them and numbering","Miscellaneous","Mooring","Inappropriate Procedure","9.19","Low","","","Stencilling & highlighting Completed","2023-06-24T23:59:35","","Completed","2023-06-05T23:59:35","No","No","No","Internal","complete as planned and close out"]
[null,null,null,30271,98288,"48_Sat Jun 03 2023 17:20:23 GMT+0800","2023-05-25T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","EGCS and accom external some light fittings rusted & broken","Miscellaneous","General Appearance","Inappropriate Procedure","","","","","De rusted & painted, Renewed the Broken light fitting on Stbd side OF EGCS Tower","2023-06-24T23:59:35","","Completed","2023-06-07T23:59:35","No","No","No","Internal","complete as planned and close out"]
[null,null,null,30273,28463,"48_Sat Jun 03 2023 17:46:12 GMT+0800","2023-05-25T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","BWTS electrolyzer leaks from feeder bolts to rectify","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.8","Medium","","","Opened & Checked all feeder bolt condition, spare received while passing Singapore all necessary parts replaced with new ones and leaks rectified..","2023-08-28T23:59:35","STAI230130 - BALLAST WATER TREATMENT SYSTEM  -  ELECTROLYSIS UNIT","Completed","2023-08-26T23:59:35","No","No","No","Internal","spares processed for supply. complete on priority on receipt of spares"]
[null,null,null,30275,45485,"48_Sat Jun 03 2023 17:53:10 GMT+0800","2023-05-25T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Some old brackets , Supports, pipelines on main deck for the previous BWTS plant to remove","Deck - Pipe / Fittings","General Appearance","Inappropriate Procedure","11.4","Very High","",""," Cropped & removed the old supports, pipes & fittings on main deck","2023-06-24T23:59:35","","Completed","2023-06-01T23:59:35","No","No","No","Internal","complete as planned and close out"]
[null,null,null,30277,82600,"48_Sat Jun 03 2023 17:06:39 GMT+0800","2023-05-25T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","IG Deck seal gauge glass to be cleaned as level was not visible.","Inert Gas","Cargo / Ballast Systems","Equipment Related","8.27","Medium","","","Opened & cleaned","2023-06-04T23:59:35","","Completed","2023-05-26T23:59:35","No","No","No","Internal"]
[null,null,null,30279,30288,"48_Sat Jun 03 2023 17:58:58 GMT+0800","2023-05-25T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Midship deck stores to arrange and stencil all the important equipment.","Miscellaneous","General Appearance","Inappropriate Procedure","11.3","Medium","","","Deck stores cleaned & arranged, Highlighting carried out for the equipments stored","2023-06-04T23:59:35","","Completed","2023-05-26T23:59:35","No","No","No","Internal"]
[null,null,null,30264,50586,"48_Sat Jun 03 2023 06:00:08 GMT+0800","2023-05-27T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Mooring Winch  Valve Unit Main Block cover pressure relief valve  damage due to corrosion","Deck - Mooring Machinery","Mooring","Equipment Related","10.12","Very High","","","Complete  pressure relief valve under STAI230140 received at Corpus Christi and renewed.","2023-08-25T23:59:35","STAI230140 -   WINDLASS/MOORING WINCH W1 received at Corpus Christi.","Completed","2023-07-12T23:59:35","No","No","No","Internal","spares processed , awaiting  readines."]
[null,null,null,30450,60515,"48_Thu Jun 15 2023 21:18:11 GMT+0800","2023-06-01T23:59:35","Defect","Ship Staff","Ship Staff Insp."," Ballast  / Fresh water Tank Vent head covers ( 11 pcs ) found wasted & heavily corroded","Miscellaneous","General Appearance","Inappropriate Procedure","11.7","High","","","Fabricated & renewed",null,"","Completed","2023-06-08T23:59:35","No","No","No","Internal"]
[null,null,null,30448,60540,"48_Wed Jun 07 2023 14:58:43 GMT+0800","2023-06-02T23:59:35","Defect","Others (Eg. Insurance etc.)","Others (Eg. Insurance etc.)","Elevator non oprational due to non availabilty of spares and requires shore assistance for data adjustment after replace ment of Part.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","Spare Main Inverter received at Singapore, the same was fitted and programmed by the service technician and the elevator was made operational.\n","2023-09-28T23:59:35","RO No. STAI230142","Completed","2023-09-16T23:59:35","No","No","No","External","spares confirmed with lead time of one month, serv to arrange once spares are received"]
[null,null,null,30449,86635,"48_Thu Jun 15 2023 21:37:09 GMT+0800","2023-06-05T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Fireman Helmet for helicopter operation found damaged.","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.43","High","","","Received","2023-09-04T23:59:35","STAI230145 - SAFETY STORES @ CORPUS CHRISTI","Completed","2023-07-04T23:59:35","No","No","No","Internal","spares arranged as per vessel request, closeout on receipt."]
[null,null,null,30899,73166,"48_Fri Jun 30 2023 05:17:17 GMT+0800","2023-06-17T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Port side gangway Movable platform found wasted & holed after derusting","Deck - Machinery","ISM Related","Equipment Related","5.47","Medium","","","Fabricated & renewed the platform section plate","2023-07-16T23:59:35","","Completed","2023-06-20T23:59:35","No","No","No","Internal"]
[null,null,null,30930,15707,"48_Sun Jul 16 2023 03:05:46 GMT+0800","2023-06-25T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Fuel oil vent head cover on poop deck found wasted & holed","Miscellaneous","General Appearance","Inappropriate Procedure","11.7","High","","","Fabricated & renewed","2023-08-25T23:59:35","","Completed","2023-06-28T23:59:35","No","No","No","Internal"]
[null,null,null,31679,19293,"48_Sat Jul 29 2023 20:03:39 GMT+0800","2023-06-28T23:59:35","Defect","Ship Staff","Ship Staff Insp.","BWTS In operational for Ballasting operation. After starting Ballasting sequence, the alarm “ Rectifier start time- Out “ is activating and system shutting down","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","Spares Received, System working satisfactory","2023-09-27T23:59:35","","Completed","2023-08-28T23:59:35","No","No","No","Internal"]
[null,null,null,30929,87052,"48_Sat Jul 15 2023 04:32:40 GMT+0800","2023-06-30T23:59:35","Defect","Ship Staff","Ship Staff Insp.","D/G No.2 Unit no.6 main bearing giving high temp. alarm,  ","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.3","Medium","","","DG no.2 stopped, sensor calibrated found OK, Replaced new bearing, D/G started taken on load found all normal, still under obserrvation. ","2023-06-30T23:59:35","","Completed","2023-06-30T23:59:35","No","No","No","Internal"]
[null,null,null,30928,62847,"48_Wed Jul 05 2023 05:16:22 GMT+0800","2023-07-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Boiler no.2 shows abnormal and NO reading in ECR \" Monitor for Boiler system","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","11.4","Very High","","","RO Raised for Unisaab controller and shore technician attended at Corpus Christi and LP-2 UNISAB replaced with new one supply from Alfa laval, Installed EPRROM 6.60E and power up panel set all parameters, tested boiler in Auto mode found working satisfactory. Tested alarms for No.2 boiler working satisfactory.","2023-07-07T23:59:35","STAI230147 & STAI230148","Completed","2023-07-07T23:59:35","No","No","No","Internal"]
[null,null,null,30927,34191,"48_Sun Jul 16 2023 03:13:53 GMT+0800","2023-07-03T23:59:35","Defect","Ship Staff","Ship Staff Insp.","During Arrival port preparation, It was found that BA 35 Valve is not closing fully from Remote & local position","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.21","High","","","BA35 Valve opened, Found Seat ring damaged, Also Found Rubber coating inside pipe damaged, Found stuck between the valve & pipe caused Seat ring to damage. Seat ring Renewed.","2023-09-02T23:59:35","","Completed","2023-07-19T23:59:35","No","No","No","Internal","noted spare seat ring onboard, complete as planned and close out. raise RO for spare seat ring"]
[null,null,null,31668,58310,"48_Thu Jul 20 2023 03:55:27 GMT+0800","2023-07-14T23:59:35","Critical Equipment","Ship Staff","Ship Staff Insp.","Emergency fire pump clutch facing and Auto valve damaged.","Critical Equip.","Emgcy. Systems","Equipment Related","5.6","Low","","","The Clutch and auto valve  renewed  with new spare. The actuating piston and cylinder overhauled. The emergency fire pump tried out in ballast passage and is working satisfactorily \n","2023-09-28T23:59:35","Urgent RO No. STAI230155.","Completed","2023-09-17T23:59:35","No","No","No","Internal","job already completed at Singapore, kindly close out"]
[null,null,null,30272,81653,"48_Sat Jun 03 2023 17:36:56 GMT+0800","2023-07-20T23:59:35","Defect","Ship Staff","Ship Staff Insp.","FGDS For Ballast tanks  giving flow failure alarm from sampling points & Bypass pump for Ballast tank giving flow failure alarm. Pump room Analyser pump fail comes","Critical Equip.","Cargo / Ballast Systems","Equipment Related","8.46","Very High","","","All the sampling lines checked by blowing with air & cleared all the lines, also no leaks found, Flapper & diaphragm changed for the pump. Filters/ Flame Trap found chocked for almost all sampling points, Filters Renewed & cleaned . Bypass pump checked. Pump room FGDS System fault rectified & working well.  Now Both System are working Normal.\n","2023-10-19T23:59:35","STAI230157 - GAS SAMPLING SYS P/R SYS SAMPLING PUMP","Completed","2023-09-24T23:59:35","No","No","No","Internal","one complete pump and other spares connected at Singapore"]
[null,null,null,30265,70411,"48_Fri Jun 02 2023 21:27:43 GMT+0800","2023-07-21T23:59:35","Defect","Ship Staff","Ship Staff Insp.","VARIOUS SECTIONS OF MOORING & VRCS HYDRAULIC LINES ON DECK FOUND HEAVILY RUSTED & WASTED. SOME SECTIONS OF AIR & FW LINE ON DECK ALSO FOUND HEAVILY RUSTED.","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.4","Very High","","","RENEWAL IN PROGRESS - 31 SECTIONS OF HYDRAULIC LINES RENEWED, 4 SECTIONS OF FW & AIR LINE RENEWED.\nVRCS & MOORING LINE LENGTH - APPROX 86 MTRS, AIR LINE: 10 MTRS, FW LINE: 10 MTRS","2023-10-20T23:59:35","","Completed","2023-10-10T23:59:35","No","No","No","Internal","ongoing jobs, monitored on weekly basis.\nclose out and follow up in weekly reports piping section."]
[null,null,null,31670,84660,"48_Tue Aug 22 2023 05:28:04 GMT+0800","2023-07-21T23:59:35","Defect","Ship Staff","Nav Audit / Verification","Found air bubble in the Magnetic Compass bowl. The liquid was found to be leaking from the bottom seal.","Navigation - Others","Navigation","Equipment Related","4.7","High","","","New Spare Bowl & TMC Flux gate supplied. Same fitted by shore technician on compass stand. One Reconditioned Magnetic Compass bowl Supplied., Kept as Spare.","2023-10-20T23:59:35","","Completed","2023-09-16T23:59:35","No","No","No","Internal","New Spare bowl supplied to vessel, kindly close out"]
[null,null,null,31676,54135,"48_Sat Jul 29 2023 19:49:26 GMT+0800","2023-07-22T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Total 29 Ballast & F.W Tank Vent head covers Found wasted / holed - while de rusting & painting","Miscellaneous","General Appearance","Equipment Related","11.7","High","","","Fabrication & Renewal Completed - Total 29 Covers completed","2023-09-20T23:59:35","","Completed","2023-08-28T23:59:35","No","No","No","Internal"]
[null,null,null,31667,34843,"48_Thu Jul 27 2023 01:42:44 GMT+0800","2023-07-23T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Main engine flex view alarm for uit no. 7 as \"Firing pressure balancing offset min value reached # 7\"","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.41","Medium","","","As per makers advise the no.2 rail valve of unit#7 renewed with new spare and problem resolved.\n","2023-09-28T23:59:35","","Completed","2023-09-17T23:59:35","No","No","No","Internal","please follow up in separate mail trail, with the pending jobs and current situation."]
[null,null,null,30262,95180,"48_Sat Jun 03 2023 16:57:05 GMT+0800","2023-07-26T23:59:35","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Spare old wires and mooring tails to land next convenient port of call.","Miscellaneous","Mooring","Inappropriate Procedure","","","","","Old Wires Landed in Singapore.","2023-10-25T23:59:35","","Completed","2023-09-16T23:59:35","No","No","No","Internal","complete as planned and close out"]
[null,null,null,30274,75239,"48_Sat Jun 03 2023 17:50:33 GMT+0800","2023-07-26T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Small U bolts on hyd lines to renew , pipeline to de rust & paint","Deck - Pipe / Fittings","General Appearance","Inappropriate Procedure","11.4","Very High","","","De rusting & painting of sections & U clamps Highlighted by Superintendent Completed. Also other weaker sections & U clamps Renewal in progress. Total Approx 200 U clamps Renewed so Far.","2023-10-25T23:59:35","","Completed","2023-09-22T23:59:35","No","No","No","Internal","complete as planned and close out"]
[null,null,null,31669,33742,"48_Mon Jul 31 2023 23:19:15 GMT+0800","2023-07-29T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Forward port Anchor Windlass Hydraulic brake cylinder shaft upper part was  leaking even after changing shaft seal  due to shaft was in bad condition pitting's at the shaft was present need to replace.","Deck - Mooring Machinery","Mooring","Equipment Related","10.12","Very High","","","The upper and bottom seals of the Port anchor windlass hydraulic brake cylinder renewed with new spares. The dressing of the pitting portion of the shaft carried out. The system tried out and found no leaks. The leaks rectified.","2024-01-28T23:59:35","STA1230169","Completed","2023-12-19T23:59:35","No","No","No","Internal","spares processed for supply, awaiting connection"]
[null,null,null,31674,99195,"48_Tue Aug 22 2023 05:20:47 GMT+0800","2023-07-31T23:59:35","Observation","Ship Staff","Nav Audit / Verification","Entries in Deck Log Book were found Overwritten at 2 occasions.","Navigation - Others","Navigation","Behaviour Based,Knowledge Based","4.1","High","","","The entries were striked out, initialled and correct entries made by the relevant OOW.","2023-10-29T23:59:35","","Completed","2023-08-01T23:59:35","No","No","No","Internal"]
[null,null,null,31675,55366,"0_Tue Aug 22 2023 05:22:23 GMT+0800","2023-07-31T23:59:35","Observation","Ship Staff","Nav Audit / Verification","Information in Master Pilot Information Exchange on the Number of Anchor shackles to be used for Anchoring with Pilot onboard found missing.","Navigation - Others","Navigation","Behaviour Based,Knowledge Based","4.1","High","","","The OOW was informed about the missing information in the Master Pilot Information exchange and instructed to cross verify that all entries are made in Master Pilot Information exchange.","2023-10-29T23:59:35","","Completed","2023-08-01T23:59:35","No","No","No","Internal"]
[null,null,null,31677,67167,"48_Tue Aug 15 2023 16:28:53 GMT+0800","2023-08-13T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Main DG No.2 Unit no. 4 exhaust temp shows incorrect reading. ","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","11.4","Very High","","","Vessel received spares while passing Singapore on 28th Aug 2023 and sensor fitted in place now working satisfactory.","2023-09-03T23:59:35","STAI230183","Completed","2023-08-27T23:59:35","No","No","No","Internal"]
[null,null,null,31678,13768,"48_Tue Aug 15 2023 16:18:48 GMT+0800","2023-08-13T23:59:35","Defect","Ship Staff","Ship Staff Insp.","M/E viscotherm alarm and indication zero viscosity.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","11.4","Very High","","","With maker remote advise trouble shooting was in progress, as per advise from office viscotherm sensor exchanged with Generator now both showing correct viscosity in ECR. ","2023-09-03T23:59:35","","Completed","2023-08-19T23:59:35","No","No","No","Internal"]
[null,null,null,31673,33745,"48_Thu Aug 31 2023 20:28:35 GMT+0800","2023-08-18T23:59:35","Defect","Ship Staff","Ship Staff Insp.","EGB LP two sections temp sensors not working","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","11.4","Very High","","","The faulty sensors renewed with new spares received at Singapore on the 14th of December 2023","2024-01-18T23:59:35","STAI230213","Completed","2023-12-27T23:59:35","No","No","No","Internal","one set of spares supplied - incorrect type.\nsecond set spares processed from makers, awaiting connection."]
[null,null,null,31671,76489,"48_Thu Aug 31 2023 20:35:47 GMT+0800","2023-08-19T23:59:35","Defect","Ship Staff","Ship Staff Insp.","EGCS SW feed pump discharge Pipe in engine room develops pin hole","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","11.4","Very High","","","The vertical section of the sea water pipe of the EGCS renewed with newly fabricated pipe by the shore workshop.","2024-01-28T23:59:35","STAI230198","Completed","2023-12-15T23:59:35","No","No","No","Internal","material supplied at Singapore. Plan at the next suitable stoppage"]
[null,null,null,31672,49423,"48_Mon Sep 11 2023 08:56:30 GMT+0800","2023-09-06T23:59:35","Defect","Ship Staff","Ship Staff Insp.","During Discharging, It was found No.3 COP AUS Pneumatic Discharge valve was not operating from CCR,","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.11","Medium","","","Troubleshooting carried out. Pump room  Air signal checked, No Air signal found for the Positioner. Checked Low selector relay found faulty, Replaced with the new spare. Now valve is working satisfactory from Remote Position i.e. CCR.\n","2023-12-05T23:59:35","","Completed","2023-09-24T23:59:35","No","No","No","Internal","revert in separate mail with troubleshooting"]
[null,null,null,32002,44781,"48_Tue Oct 03 2023 16:43:33 GMT+0800","2023-09-17T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Ballast Tank Vent Head Covers found wasted & holed","Miscellaneous","General Appearance","Equipment Related","11.7","High","","","Fabrication & Renewal Completed (Total 38 Ballast Vent head covers Found wasted- Fabricated)","2023-11-17T23:59:35","","Completed","2023-10-10T23:59:35","No","No","No","Internal","complete and close out as planned"]
[null,null,null,32003,20672,"48_Tue Oct 03 2023 15:43:34 GMT+0800","2023-09-17T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Hypermist system tried out in auto/manual and found the hypermist pump starting and stooping frequently.\n\n","LSA / FFA","Eng. / Strg. Comp.","Equipment Related","5.40","Very High","","","checked the starter panel of the pump and found the soft starter body is broken and secured with the tape, same removed and checked found two wire connection broken from the PCB inside, both connections soldered and boxed back the soft starter fitted in palce auto/manual operation tried out, now working.\n","2023-11-17T23:59:35","","Completed","2023-09-18T23:59:35","No","No","No","Internal"]
[null,null,null,32004,39926,"48_Tue Oct 03 2023 15:46:21 GMT+0800","2023-09-19T23:59:35","Defect","Ship Staff","Ship Staff Insp.","The HP drum water level controller was erratic and level not maintaining . On inspection found that the diaphragm was damaged .\n","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.31","Very High","","","The damaged diaphragm renewed with new spare and the controller working satisfactory.\n\n","2023-12-19T23:59:35","","Completed","2023-09-21T23:59:35","No","No","No","Internal"]
[null,null,null,32005,67723,"48_Tue Oct 03 2023 15:48:08 GMT+0800","2023-09-23T23:59:35","Defect","Ship Staff","Ship Staff Insp.","The Mechanical seal of the fresh water hydrophore pump no.1 found leaking.\n","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.31","Very High","","","The Mechanical seal renewed and found running satisfactory without any leaks.\n","2023-12-23T23:59:35","","Completed","2023-09-25T23:59:35","No","No","No","Internal"]
[null,null,null,32001,26459,"48_Tue Oct 03 2023 16:40:32 GMT+0800","2023-09-24T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Cover/Lip of Two Natural vent (SIP ) Cover of sample & Sopep locker found wasted During De rusting","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.8","Low","","","Fabricated & Renewed","2023-11-23T23:59:35","","Completed","2023-10-07T23:59:35","No","No","No","Internal","complete and close out as planned"]
[null,null,null,33428,95973,"48_Mon Dec 11 2023 08:31:52 GMT+0800","2023-10-15T23:59:35","Defect","Ship Staff","Ship Staff Insp.","4 No.s Ballast Air Vent Head Floats (stainless steel)  found broken  (FPK & 1W) ","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.7","High","","","All 4 Floats Renewed after receiving the spares","2024-01-14T23:59:35","","Completed","2023-12-08T23:59:35","No","No","No","Internal"]
[null,null,null,32374,66015,"48_Tue Oct 31 2023 06:31:27 GMT+0800","2023-10-27T23:59:35","Defect","Ship Staff","Ship Staff Insp.","The Insulation of the Power Cable of the Engine room overhead crane brittle and broken at various locations and the same giving out 440 V low insulation alarm when operating the crane.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","11.4","Very High","","","The Power cable of the Engine room crane renewed with the new spare cable as the old cable was giving out 440V low insulation alarm. The crane has been tested and is found working satisfactory.","2024-03-15T23:59:35","STAI230259 ENGINE ROOM CRANE CABLES","Completed","2024-02-10T23:59:35","No","No","No","Internal","spares onboard, kindly complete and close out"]
[null,null,null,32526,24445,"48_Fri Nov 03 2023 19:09:31 GMT+0800","2023-10-30T23:59:35","Defect","Ship Staff","Ship Staff Insp.","BWTS Filter Inlet Valve BT-1211, Not Operating Remotely/On Auto, Need to Operate Locally From Pump room, As the magnetic switch (local/remote/latch), got brittle and the magnet is missing, hence the valve is holding at local mode by default.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.11","Medium","","","Troubleshooting carried out, Requisition raised for spare.  Temporarly we have put it on Remote mode using A magnet on the valve in place of the switch. Now it can be operated remotely / Auto","2024-04-29T23:59:35","STAI230251 BWTS FILTER UNIT INLET VALVE","Completed","2024-01-10T23:59:35","No","No","No","Internal","vv made operational with ecternal magnet"]
[null,null,null,32527,95476,"48_Sun Nov 05 2023 15:27:51 GMT+0800","2023-11-04T23:59:35","Defect","Ship Staff","Ship Staff Insp.","The Port side HFO bunker manifold valve defective and needs to be renewed. The valve presently in shut position.","Deck - Pipe / Fittings","General Appearance","Equipment Related","6.8","High","","","The Defective valve has been renewed with new spare valve.","2024-04-04T23:59:35","STAI230231  ENGINE STORES","Completed","2024-02-13T23:59:35","No","No","No","Internal","stores received onboard, please complete  and close out"]
[null,null,null,35344,91130,"0_Fri May 24 2024 22:10:13 GMT+0800","2023-12-14T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","1C COT COW root valve to overhaul","Deck - Machinery","Cargo / Ballast Systems","Equipment Related","8.34","High","","","COW root valve overhauled","2024-01-13T23:59:35","","Completed","2023-12-20T23:59:35","No","No","No","Internal"]
[null,null,null,35345,64696,"0_Fri May 24 2024 22:11:09 GMT+0800","2023-12-14T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Slop port IG isolation valve to overhaul","Deck - Pipe / Fittings","","Equipment Related","8.50","Medium","","","Valve overhauled and lubricated","2024-01-13T23:59:35","","Completed","2023-12-22T23:59:35","No","No","No","Internal"]
[null,null,null,35347,86274,"0_Fri May 24 2024 22:12:01 GMT+0800","2023-12-14T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Derusting and painting of foam monitor stands and pipelines beneath","Deck - Pipe / Fittings","General Appearance","Equipment Related","5.38","High","","","Foam monitor stands and pipelines beneath de-rusted and painted","2024-03-13T23:59:35","","Completed","2024-01-11T23:59:35","No","No","No","Internal"]
[null,null,null,35348,55234,"0_Fri May 24 2024 22:12:52 GMT+0800","2023-12-14T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Cargo tank overfill high level alarms stenciling to carry out","Miscellaneous","","Behaviour Based","11.4","Very High","","","Overfill alarm stenciling carried out","2024-01-13T23:59:35","","Completed","2023-12-25T23:59:35","No","No","No","Internal"]
[null,null,null,35349,55529,"48_Fri May 24 2024 22:19:56 GMT+0800","2023-12-14T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Main deck Helicopter landing area to spot chip and paint","Miscellaneous","Structural Condn. / WT integrity ","Human Error","11.4","Very High","","","Spot chipping and painting carried out","2023-12-23T23:59:35","","Completed","2023-12-20T23:59:35","No","No","No","Internal"]
[null,null,null,35353,17594,"0_Fri May 24 2024 22:15:46 GMT+0800","2023-12-14T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Slop port IG isolation valve to overhaul","Deck - Pipe / Fittings","","Equipment Related","8.50","Medium","","","Valve overhauled and lubricated","2024-01-13T23:59:35","","Completed","2023-12-22T23:59:35","No","No","No","Internal"]
[null,null,null,35354,53314,"48_Fri May 24 2024 22:18:46 GMT+0800","2023-12-14T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Scrubber tower casing to spot de rust and paint","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","11.4","Very High","","","De-rusted and painted","2024-01-13T23:59:35","","Completed","2024-01-09T23:59:35","No","No","No","Internal"]
[null,null,null,35368,30539,"0_Fri May 24 2024 23:26:44 GMT+0800","2023-12-14T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Spare Vertical Pipe section for the EGCS Sea water line to fabricate and keep standby","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","SPARE VERTICAL PIPE FOR EGCS FABRICATED AND KEPT STANDBY FOR INSTALLATION. ","2024-03-14T23:59:35","","Completed","2024-01-15T23:59:35","No","No","No","Internal"]
[null,null,null,35370,16336,"0_Fri May 24 2024 23:30:24 GMT+0800","2023-12-14T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","EGCS Inventory to Update","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Spare parts physical inventory taken, and ROB updated in PAL. ","2023-12-29T23:59:35","","Completed","2024-03-02T23:59:35","No","No","No","Internal"]
[null,null,null,35371,41584,"0_Fri May 24 2024 23:32:05 GMT+0800","2023-12-14T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Aux DG Exhaust Manifold gaskets and bellows to renew, exhaust leaks to rectify","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Aux DG, leaking exhaust manifold Bellows and gaskets replaced with newly recieved spares. All exhaust leaks rectified. ","2023-12-29T23:59:35","","Completed","2023-12-21T23:59:35","No","No","No","Internal"]
[null,null,null,35373,39964,"0_Fri May 24 2024 23:33:42 GMT+0800","2023-12-14T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","HP Drum gauge glass (stbd) gland leak to rectify","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Gland packing renewed and Leak rectified. ","2023-12-29T23:59:35","","Completed","2024-01-23T23:59:35","No","No","No","Internal"]
[null,null,null,35375,69562,"0_Fri May 24 2024 23:28:08 GMT+0800","2023-12-14T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Newly fitted PAH Sensor for EGCS Effluent to secure","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","","10.32","Very High","","","","2023-12-21T23:59:35","","Completed","2023-12-20T23:59:35","No","No","No","Internal"]
[null,null,null,35381,16380,"0_Fri May 24 2024 23:35:19 GMT+0800","2023-12-14T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","\tMain DG#1 T/C Sealing air line wasted ferrule to renew","E/R - Main Engine,E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Ferrule renewed and leak rectified. ","2023-12-29T23:59:35","","Completed","2024-02-09T23:59:35","No","No","No","Internal"]
[null,null,null,35400,78236,"0_Fri May 24 2024 23:23:06 GMT+0800","2023-12-14T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","","2024-03-14T23:59:35","EGB Defective Soot blower Lances to renew","Completed","2023-12-26T23:59:35","No","No","No","Internal"]
[null,null,null,33730,89436,"48_Tue Jan 16 2024 18:30:36 GMT+0800","2023-12-20T23:59:35","Observation","Ship Staff","Ship Staff Insp.","2 C & SLOP PORT IG ISOLATION VALVE unable to close properly","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.2","Medium","","","2 C & SLOP PORT IG ISOLATION VALVE Overhauled and are now operating satisfactorily","2024-03-19T23:59:35","","Completed","2023-12-22T23:59:35","No","No","No","Internal"]
[null,null,null,32528,47478,"48_Sun Nov 05 2023 15:33:45 GMT+0800","2023-12-27T23:59:35","Defect","Ship Staff","Ship Staff Insp.","The EGB drain valve is fully corroded and needs to be renewed.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","EGB drain valve renewed with spare recieved onboard. ","2024-05-15T23:59:35","","Completed","2024-04-19T23:59:35","No","No","No","Internal","complete and close out as planned, at Long beach - stores rcd onboard"]
[null,null,null,35350,21143,"48_Fri May 24 2024 22:21:00 GMT+0800","2023-12-28T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Crew recreation room sofa chair upholstery torn","Accommodation","General Appearance","Behaviour Based","","","","","Upholstery repaired in crew recreation room","2024-03-28T23:59:35","","Completed","2024-03-24T23:59:35","No","No","No","Internal"]
[null,null,null,33429,58951,"48_Fri Jan 12 2024 20:45:17 GMT+0800","2024-01-02T23:59:35","Defect","Ship Staff","Ship Staff Insp.","IGS Deck Seal Pump NO.1 Mechanical seal Leaking","Inert Gas","Eng. / Strg. Comp.","Equipment Related","10.31","Very High","","","The Mechanical Seal renewed with spare new mechanical seal, the leak rectified.","2024-04-02T23:59:35","","Completed","2024-01-12T23:59:35","No","No","No","Internal"]
[null,null,null,33728,98299,"48_Tue Jan 16 2024 18:32:05 GMT+0800","2024-01-12T23:59:35","Observation","Ship Staff","Ship Staff Insp.","No. 1 WBT eductor valves BA005 & BA 006 unable to operate from CCR","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.21","High","","","The  operation of the valves have been tried out remotely from CCR and is found to be working satisfactory , Did not observe any major issue with regards to the operation.","2024-04-11T23:59:35","","Completed","2024-01-17T23:59:35","No","No","No","Internal"]
[null,null,null,33727,98324,"48_Wed Jan 17 2024 13:40:17 GMT+0800","2024-01-13T23:59:35","Defect","Ship Staff","Ship Staff Insp.","The Main Engine rpm indicator ( Stbd) bridge wing sluggish and erratic.","Navigation - Others","Navigation","Equipment Related","4.7","High","","","RPM INDICATOR REPAIRED BY SHIP STAFF TESTED WORKING SATISFACTORY ","2024-04-28T23:59:35","STAI240023","Completed","2024-04-28T23:59:35","No","No","No","Internal","will be processed as per request, upon receipt of quotes"]
[null,null,null,33729,30788,"48_Wed Jan 17 2024 13:50:31 GMT+0800","2024-01-13T23:59:35","Defect","Ship Staff","Ship Staff Insp.","The Salinity Indicator found burnt giving out 440V low insulation alarm.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","replaced with spare received. Working fine now","2024-04-13T23:59:35","STAI240013","Completed","2024-03-04T23:59:35","No","No","No","Internal","spares connected at Long Beach 29 Feb. Complete and close out"]
[null,null,null,33747,62916,"48_Wed Jan 31 2024 05:44:01 GMT+0800","2024-01-14T23:59:35","Defect","Ship Staff","Ship Staff Insp.","The No.1 N.A. Pump of the BWTS non operational. The BLDC motor driver needs to be replaced.","Deck - Machinery","Cargo / Ballast Systems","Equipment Related","8.11","Medium","","","The BLDC motor driver replaced with the new spare recieved in Long beach. Installed in place and operational test run done, satisfactorily. ","2024-04-13T23:59:35","STAI235067.","Completed","2024-03-18T23:59:35","No","No","No","Internal","processed for supply"]
[null,null,null,33746,41903,"48_Wed Jan 31 2024 05:51:24 GMT+0800","2024-01-26T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","The Purifier sump oil sight glass gave away and the sump oil was lost which lead to the lack of lubrication damaging the bearing and the shaft.","E/R - Purifier","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Spares recieved onboard. Complete shaft overhaul of Purifier carried out with new shaft , bearings  and neck bearing assembly.  New sump oil sight glass fixed in place. Purifier boxed back and run. Running well, satisfactorily. All parameters normal. No vibrations. ","2024-04-25T23:59:35","","Completed","2024-03-08T23:59:35","No","No","No","Internal","include RO number in DDRL and complete the job on priority after receiving spares at LB."]
[null,null,null,33745,23109,"48_Thu Feb 01 2024 12:30:27 GMT+0800","2024-01-27T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Main Engine remote control communication alarms getting activated continuously on the ACP of bridge and ECR, these are non critical alarms and the Main engine is running satisfactory.","Navigation - Others","Navigation","Equipment Related","4.7","High","","","PSS 1B Card renewed. Working satisfactorily now without any alarms. ","2024-04-26T23:59:35","","Completed","2024-04-14T23:59:35","No","No","No","Internal","make service RO for next call Singapore."]
[null,null,null,33998,30564,"48_Thu Feb 15 2024 23:16:40 GMT+0800","2024-02-05T23:59:35","Defect","Ship Staff","Ship Staff Insp.","The Motor controller of the Fire and Bilge Pump No.2 faulty and as such the pump unable to stop from Bridge nor from the engine room.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","11.4","Very High","","","The Motor controller renewed with new spare and tried out, found working satisfactory.","2024-05-02T23:59:35","","Completed","2024-02-07T23:59:35","No","No","No","Internal"]
[null,null,null,34449,58811,"48_Sun Mar 03 2024 09:01:46 GMT+0800","2024-02-18T23:59:35","Defect","Ship Staff","Ship Staff Insp.","THE Pressure transmitter of the BWTS  no.1 autoflushing filter (inlet transmitter) defective.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.11","Medium","","","The defective Pressure transmitter renewed with the transmitter taken from the aft Peak tank BWTS filter unit. The system working satisfactory.","2024-05-18T23:59:35","STAI240061","Completed","2024-04-28T23:59:35","No","No","No","Internal","BWTS is planned upgrade to Non filter this year.\nspares to be arranged as requested.\njob completed as per action comments"]
[null,null,null,35339,54983,"0_Fri May 24 2024 22:02:50 GMT+0800","2024-02-28T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Salinity Indicator for Fresh water generator No:2 is damaged. Need to be replaced. Awaiting spare.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","replaced with spare received. Working fine now","2024-04-28T23:59:35","","Completed","2024-03-04T23:59:35","No","No","No","Internal"]
[null,null,null,35340,53090,"0_Fri May 24 2024 22:05:13 GMT+0800","2024-02-28T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Wheel house AC – belt found broken, to be renewed","Accommodation","","Equipment Related","","","","","Belt Renewed. ","2024-04-28T23:59:35","","Completed","2024-03-05T23:59:35","No","No","No","Internal"]
[null,null,null,35341,13619,"0_Fri May 24 2024 22:06:30 GMT+0800","2024-02-28T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Hot water Calorifier steam return line valve wheel is missing. To be put in place.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Behaviour Based","10.32","Very High","","","NEW VALVE INSTALLED IN PLACE.","2024-03-28T23:59:35","","Completed","2024-03-03T23:59:35","No","No","No","Internal"]
[null,null,null,35342,39840,"0_Fri May 24 2024 22:04:00 GMT+0800","2024-02-28T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","One damaged and bandaged air hose found still in use in ER workshop. To be replaced.  ","Miscellaneous","Eng. / Strg. Comp.","Human Error","10.29","Medium","","","HOSE REPLACED WITH NEW","2024-03-07T23:59:35","","Completed","2024-03-06T23:59:35","No","No","No","Internal"]
[null,null,null,35343,32783,"0_Fri May 24 2024 22:07:39 GMT+0800","2024-02-28T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Stbd Side midship crane starting box panel grounding cable broken","Deck - Machinery","Cargo / Ballast Systems","Equipment Related","8.73","Medium","","","Grounding wire fixed back in place. ","2024-03-28T23:59:35","","Completed","2024-03-21T23:59:35","No","No","No","Internal"]
[null,null,null,35346,53145,"48_Fri May 24 2024 22:01:55 GMT+0800","2024-02-28T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","The No.1 N.A. Pump of the BWTS nonoperational. The BLDC motor driver needs to be replaced.","Miscellaneous","Cargo / Ballast Systems","Equipment Related","8.11","Medium","","","The BLDC motor driver replaced with the new spare recieved in Long beach. Installed in place and operational test run done, satisfactorily. ","2024-04-28T23:59:35","","Completed","2024-03-18T23:59:35","No","No","No","Internal"]
[null,null,null,35351,77344,"0_Fri May 24 2024 22:22:03 GMT+0800","2024-02-28T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Manifold reducers require maintenance as flanges showing corrosion and rust spots","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","Behaviour Based","8.41","Medium","","","Manifold reducers de-rusted and painted. ","2024-04-28T23:59:35","","Completed","2024-03-27T23:59:35","No","No","No","Internal"]
[null,null,null,35352,91632,"0_Fri May 24 2024 22:22:51 GMT+0800","2024-02-28T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Steam coils blanks for both slop tanks to de-rust and paint","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","Equipment Related","8.15","High","","","Steam coils de-rusted and painted","2024-03-19T23:59:35","","Completed","2024-02-29T23:59:35","No","No","No","Internal"]
[null,null,null,35355,56956,"0_Fri May 24 2024 22:26:31 GMT+0800","2024-02-28T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Bosun store mechanical vent emergency stop switch board detached from the main frame","Deck - Pipe / Fittings","","","11.8","Low","","","Switch board fixed back in position, frame de-rusted and painted","2024-03-28T23:59:35","","Completed","2024-03-24T23:59:35","No","No","No","Internal"]
[null,null,null,35356,31516,"0_Fri May 24 2024 22:34:18 GMT+0800","2024-02-28T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Stbd side mid-ship crane operating platform grating found to be corroded","Deck - Pipe / Fittings","General Appearance","","8.73","Medium","","","Stbd Side mid-ship hose handling crane operating platform grating renewed","2024-03-28T23:59:35","","Completed","2024-03-16T23:59:35","No","No","No","Internal"]
[null,null,null,35357,42987,"48_Fri May 24 2024 22:35:19 GMT+0800","2024-02-28T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","WBT no 1, 2 & 3 tank entrance area spot de-rusting / painting required","Miscellaneous","","","2.16","Medium","","","WBT no 1,2&3 tank Entrance area de-rusted and painted","2024-04-28T23:59:35","","Completed","2024-03-22T23:59:35","No","No","No","Internal"]
[null,null,null,35358,20225,"0_Fri May 24 2024 22:37:32 GMT+0800","2024-02-28T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Bosun Store Davit found to be rusted. De-rusting/painting to be carried out for the same","Miscellaneous","Structural Condn. / WT integrity ","","11.8","Low","","","De-rusting and painting  carried out","2024-03-28T23:59:35","","Completed","2024-03-08T23:59:35","No","No","No","Internal"]
[null,null,null,35359,75353,"0_Fri May 24 2024 22:23:43 GMT+0800","2024-02-28T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","FW Valve on E-deck stbd side accom wasted. ","Deck - Pipe / Fittings","","","11.4","Very High","","","FW valve on E-deck de-rusted and painted","2024-03-09T23:59:35","","Completed","2024-03-01T23:59:35","No","No","No","Internal"]
[null,null,null,35360,90956,"0_Fri May 24 2024 22:36:22 GMT+0800","2024-02-28T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Both anchor chains Spurling Pipe area heavy flakes of rust present","Miscellaneous","General Appearance","","11.8","Low","","","Spurling pipes de-rusted and painted.","2024-04-28T23:59:35","Both anchor chains Spurling Pipe area heavy flakes of rust present","Completed","2024-03-26T23:59:35","No","No","No","Internal"]
[null,null,null,35361,13472,"0_Fri May 24 2024 22:25:38 GMT+0800","2024-02-28T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Upper deck accommodation entrance fresh water line valve wheel found to be broken","Deck - Pipe / Fittings","","","11.8","Low","","","Valve Wheel renewed","2024-03-28T23:59:35","","Completed","2024-03-24T23:59:35","No","No","No","Internal"]
[null,null,null,35362,33906,"0_Fri May 24 2024 22:38:12 GMT+0800","2024-02-28T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Both Hose Handling cranes to be de-rusted spot painting to be carried out for the same","Miscellaneous","Structural Condn. / WT integrity ","","11.8","Low","","","De-rusting and painting carried out","2024-03-28T23:59:35","","Completed","2024-03-01T23:59:35","No","No","No","Internal"]
[null,null,null,35363,53675,"0_Fri May 24 2024 22:24:44 GMT+0800","2024-02-28T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Air Line Cap for deck air line near pump room entrance found to be missing","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","","11.4","Very High","","","Air line Cap placed back and secured","2024-03-08T23:59:35","","Completed","2024-03-04T23:59:35","No","No","No","Internal"]
[null,null,null,35364,23048,"0_Fri May 24 2024 22:38:54 GMT+0800","2024-02-28T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Mooring Winch no 5 need to be de-rusted","Miscellaneous","Structural Condn. / WT integrity ","","","","","","De-rusting and painting carried out","2024-04-28T23:59:35","","Completed","2024-03-29T23:59:35","No","No","No","Internal"]
[null,null,null,35365,30678,"0_Fri May 24 2024 22:39:47 GMT+0800","2024-02-28T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Main deck DO Filling line has scattered rust and wastage","Miscellaneous","Structural Condn. / WT integrity ","","","","","","De-rusting and painting carried out","2024-03-29T23:59:35","","Completed","2024-03-28T23:59:35","No","No","No","Internal"]
[null,null,null,35366,98538,"0_Fri May 24 2024 22:40:33 GMT+0800","2024-02-28T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Snap back zones to have larger, more conspicuous warning notices stencilled ","Miscellaneous","","","9.8","Medium","","","Re-marking of Snap Back zones carried out.","2024-03-29T23:59:35","","Completed","2024-03-29T23:59:35","No","No","No","Internal"]
[null,null,null,35367,59922,"0_Fri May 24 2024 22:41:58 GMT+0800","2024-02-28T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Both Sides life rafts securing chains rusted.","Miscellaneous","Structural Condn. / WT integrity ","","5.15","Medium","","","Derusted and Painted","2024-03-09T23:59:35","","Completed","2024-03-06T23:59:35","No","No","No","Internal"]
[null,null,null,35369,82574,"48_Fri May 24 2024 22:00:19 GMT+0800","2024-02-28T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","HFO Purifier No:1 shaft damaged. Awaiting spares.","E/R - Purifier","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Spares recieved onboard. Complete shaft overhaul of Purifier carried out with new shaft , bearings  and neck bearing assembly.  New sump oil sight glass fixed in place. Purifier boxed back and run. Running well, satisfactorily. All parameters normal. No vibrations. ","2024-04-28T23:59:35","","Completed","2024-03-08T23:59:35","No","No","No","Internal"]
[null,null,null,35372,16014,"48_Fri May 24 2024 23:21:23 GMT+0800","2024-02-28T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Fwd life raft area IMO symbols faded","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.31","High","","","Imo symbol replaced with new one\n","2024-03-28T23:59:35","","Completed","2024-03-26T23:59:35","No","No","No","Internal"]
[null,null,null,35374,46864,"0_Fri May 24 2024 23:24:50 GMT+0800","2024-02-28T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","2 Remote hydraulic operating valves in E.R 3rd deck to be stencilled/marked for easy identification.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","","10.29","Medium","","","STENCILLING DONE.  BOTH REMOTE HYDRAULIC VALVES ARE WELL MARKED FOR EASY IDENTIFICATION. ","2024-03-28T23:59:35","","Completed","2024-03-20T23:59:35","No","No","No","Internal"]
[null,null,null,35376,68821,"48_Fri May 24 2024 23:45:34 GMT+0800","2024-02-28T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Main Engine remote control communication alarms getting activated continuously on the ACP of bridge and ECR, these are noncritical alarms and the Main engine is running satisfactory.","Navigation - Others","Navigation","Equipment Related","10.32","Very High","","","PSS 1B Card renewed. Working satisfactorily now without any alarms. ","2024-04-28T23:59:35","","Completed","2024-04-14T23:59:35","No","No","No","Internal"]
[null,null,null,35377,27882,"0_Fri May 24 2024 23:47:20 GMT+0800","2024-02-28T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","EGB drain valve is corroded and hard to operate. To be overhauled/renewed. ","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","EGB drain valve renewed with spare received onboard. ","2024-03-28T23:59:35","","Completed","2024-04-19T23:59:35","No","No","No","Internal"]
[null,null,null,35378,38093,"48_Fri May 24 2024 23:50:08 GMT+0800","2024-02-28T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Stbd side Midship crane operating lever rusted and wasted","Deck - Pipe / Fittings","General Appearance","Equipment Related","8.73","Medium","","","Operating Levers renewed and replaced with new one","2024-04-28T23:59:35","","Completed","2024-04-23T23:59:35","No","No","No","Internal"]
[null,null,null,35380,77462,"0_Fri May 24 2024 22:09:11 GMT+0800","2024-02-28T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Stbd Side midship DO Drain Line valve wheel broken.","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","Equipment Related","8.41","Medium","","","Valve hand wheel renewed. ","2024-03-28T23:59:35","","Completed","2024-03-02T23:59:35","No","No","No","Internal"]
[null,null,null,35382,22230,"48_Fri May 24 2024 23:43:08 GMT+0800","2024-02-28T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Tube lights on top of BWTS room are out. To be renewed. ","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","LIGHTS RENEWED. ","2024-03-10T23:59:35","","Completed","2024-04-05T23:59:35","No","No","No","Internal"]
[null,null,null,35388,95186,"0_Sat May 25 2024 00:52:00 GMT+0800","2024-02-28T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","The Main Engine RPM indicator (Stbd) bridge wing sluggish and erratic.","Navigation - Others","Navigation","Equipment Related","4.7","High","","","RPM INDICATOR REPAIRED BY SHIP STAFF TESTED WORKING SATISFACTORY ","2024-04-28T23:59:35","","Completed","2024-04-28T23:59:35","No","No","No","Internal"]
[null,null,null,35396,23318,"48_Sat May 25 2024 00:56:36 GMT+0800","2024-02-28T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","No 1 DGPS is showing the FLash ROM2 access error keeps popping up intermittently and goes off on its own","Navigation - RADAR","Navigation","Equipment Related","4.7","High","","","NEW DGPS INSTALLED TESTED  WORKING SATISFACTORY.","2024-04-28T23:59:35","","Completed","2024-03-07T23:59:35","No","No","No","Internal"]
[null,null,null,35325,33085,"0_Fri May 24 2024 19:26:24 GMT+0800","2024-02-28T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","One of the calorifer heater-heating elements was giving low inulation. The sane has been disconencted and requistion made for same.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","heater element changed. Working satisfactory.","2024-05-28T23:59:35","","Completed","2024-05-29T23:59:35","No","No","No","Internal"]
[null,null,null,35389,43731,"0_Sat May 25 2024 00:54:44 GMT+0800","2024-04-03T23:59:35","Defect","Ship Staff","Ship Staff Insp.","M.E F.O VISCOSITY CONTROLLER WORKS ERRATICALLY. ","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Changed interface box and sensor . . SHOWING CORRECT VISCOSITY","2024-05-25T23:59:35","","Completed","2024-05-08T23:59:35","No","No","No","Internal"]
[null,null,null,35331,98834,"0_Fri May 24 2024 19:39:43 GMT+0800","2024-04-16T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","OWS CHAMBER LEAK TO RECTIFY","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","EMULSION TANK IS LEAKING ( FITTED ON THE OIL SEPARATION STAGE TANK )FROM THE WELDING. NEED TO REMOVE THE TANK AND DO WELDING","2024-05-30T23:59:35","","Completed","2024-05-26T23:59:35","No","No","No","Internal","job completed as per weekly report 26th May"]
[null,null,null,35336,41199,"0_Sat May 25 2024 00:44:49 GMT+0800","2024-04-16T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Both boilers aft side to clean and apply fresh paint.","Miscellaneous","Eng. / Strg. Comp.","","10.32","Very High","","","Boiler cleaned and painted","2024-07-13T23:59:35","","Completed","2024-05-29T23:59:35","No","No","No","Internal","complete and close out before 31st May"]
[null,null,null,35337,67818,"0_Fri May 24 2024 19:42:16 GMT+0800","2024-04-16T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","TOP FOUR CABINS CURTAINS TO INSTALL AND REMOVE THE MAKE SHIFT ARRANGEMENT","Accommodation","","Inappropriate Procedure","","","","","BLIND ASSEMBLE FOR CURTAINS Requested in Stores, Reference number STAI 240141","2024-07-16T23:59:35","","Completed","2024-05-28T23:59:35","No","No","No","Internal","raise RO for required material and close out"]
[null,null,null,35338,38307,"0_Fri May 24 2024 19:43:21 GMT+0800","2024-04-16T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","BOTH WINDLASS OUTER DRUMS , INNER BEARINGS SLEEVES worn out","Deck - Mooring Machinery","Mooring","Equipment Related","","","","","JOB SHIFTED TO REFMAN","2024-07-15T23:59:35","","Completed","2024-05-28T23:59:35","No","No","No","Internal","forward the REFMAN defect asap."]
[null,null,null,35379,95639,"0_Sat May 25 2024 00:38:39 GMT+0800","2024-04-16T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Crew laundry drain line clogged on sunken deck.","Accommodation","Eng. / Strg. Comp.","","11.3","Medium","","","Drain pipeline removed and cleared.","2024-04-15T23:59:35","","Completed","2024-04-15T23:59:35","No","No","No","Internal"]
[null,null,null,35383,47842,"0_Sat May 25 2024 00:40:14 GMT+0800","2024-04-16T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","\tWHRS sootblower glands to lubricate with graphite grease\n\n","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","",""," glands to lubricate with graphite grease","2024-04-23T23:59:35","","Completed",null,"No","No","No","Internal"]
[null,null,null,35384,13742,"0_Sat May 25 2024 00:43:33 GMT+0800","2024-04-16T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Stbd boiler steam leak after steam isolation valve.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Leak rectified","2024-04-16T23:59:35","","Completed","2024-04-13T23:59:35","No","No","No","Internal"]
[null,null,null,35385,23370,"0_Sat May 25 2024 00:46:06 GMT+0800","2024-04-16T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ME air cooler sight glasses to clean.","E/R - Main Engine,E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","","2024-05-15T23:59:35","","Completed","2024-04-14T23:59:35","No","No","No","Internal"]
[null,null,null,35386,61349,"0_Sat May 25 2024 00:49:04 GMT+0800","2024-04-16T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","BA compressor, no seperate relief valve for lifeboat bottle charging. Procedures to be corrected for adjustment of blow off valve\n\n","LSA / FFA","Eng. / Strg. Comp.","Equipment Related","","","","","Procedures corrected and posted in foam room","2024-04-30T23:59:35","","Completed","2024-04-19T23:59:35","No","No","No","Internal"]
[null,null,null,35387,83261,"0_Sat May 25 2024 00:50:18 GMT+0800","2024-04-16T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","LO purifier heater not maintaining 95 degree C, heater to clean regularly as pe PMS every 3M","E/R - Purifier","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","LO purifier heater taken out and cleaned. Now purifier maintaining 95 degree C.","2024-05-30T23:59:35","","Completed","2024-05-06T23:59:35","No","No","No","Internal"]
[null,null,null,35390,92976,"0_Sat May 25 2024 00:47:36 GMT+0800","2024-04-16T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","COPT Gov links and steam control vv stem to lubricate with molycote regularly.\n\n","Cargo Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","COPT Gov links and steam control vv stem  lubricated with molycote.\n\n","2024-04-30T23:59:35","","Completed","2024-04-20T23:59:35","No","No","No","Internal"]
[null,null,null,35391,39105,"0_Sat May 25 2024 01:25:06 GMT+0800","2024-04-16T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ER FW plate type coolers, studs and ratchet to derust & grease. Renew defective SW pr gauges.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","ER FW plate type coolers, studs and ratchet cleaned and greased..  Renewed defective FW pr gauges. (2 nos)","2024-05-15T23:59:35","","Completed","2024-05-15T23:59:35","No","No","No","Internal"]
[null,null,null,35392,43235,"0_Fri May 24 2024 19:38:38 GMT+0800","2024-04-16T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ME HFO PUMP LUB EOIL LINES TO FLUSH WITH WD40 AS PER MAKERS INSTRUCTIONS AT SINGAPORE WHILE BUNKERING","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","ME FO PUMP #1,2,3 FLUSHING CARRIED OUT AT SINGAPORE BY SHORE PERSONNEL","2024-05-15T23:59:35","","Completed","2024-04-29T23:59:35","No","No","No","Internal"]
[null,null,null,35393,34360,"0_Sat May 25 2024 00:53:22 GMT+0800","2024-04-16T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Battery isolators missing from both the boat batteries.","Miscellaneous","Safety / LSA / FFA","Equipment Related","5.29","High","","","BOTH LIFE BOAT HAVE BATTERY ISOLATERS","2024-05-10T23:59:35","","Completed","2024-05-04T23:59:35","No","No","No","Internal"]
[null,null,null,35394,94347,"0_Sat May 25 2024 00:41:51 GMT+0800","2024-04-16T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ME LO auto Boll filter oil leaks; gauge to renew.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Leak recified and gauge renewed","2024-04-23T23:59:35","","Completed","2024-04-19T23:59:35","No","No","No","Internal"]
[null,null,null,35398,49861,"0_Sat May 25 2024 01:11:12 GMT+0800","2024-04-16T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","BA compressor, no seperate relief valve for lifeboat bottle charging. Procedures to be corrected for adjustment of blow off valve","LSA / FFA","Eng. / Strg. Comp.","Equipment Related","10.16","Very High","","","BA compressor, no seperate relief valve for lifeboat bottle charging. Procedures corrected for adjustment of blow off valve prior charging lifeboat air bottles.","2024-05-15T23:59:35","","Completed","2024-05-02T23:59:35","No","No","No","Internal"]
[null,null,null,35399,87042,"0_Sat May 25 2024 01:12:39 GMT+0800","2024-04-16T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Boiler spare burners to OH and seal oil holes with cling wrap.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Aux. Boiler spare pilot and main burners overhauled and oil holes sealed with cling wrap.","2024-04-23T23:59:35","","Completed","2024-04-21T23:59:35","No","No","No","Internal"]
[null,null,null,35401,40231,"0_Sat May 25 2024 01:23:41 GMT+0800","2024-04-16T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Port Pilot Ladder winch gear box seal leak","Deck - Machinery","ISM Related","Equipment Related","","","","","Seal leak rectified and oil Renewed","2024-04-30T23:59:35","","Completed","2024-04-26T23:59:35","No","No","No","Internal"]
[null,null,null,35690,73738,"48_Sat Jun 01 2024 00:59:32 GMT+0800","2024-04-16T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Ship specific detailed UMS checklist not is use, to implement.","Miscellaneous","Eng. / Strg. Comp.","Inappropriate Procedure","10.32","Very High","","","put in use","2024-04-23T23:59:35","","Completed","2024-04-18T23:59:35","No","No","No","Internal"]
[null,null,null,35691,95010,"48_Sat Jun 01 2024 00:24:30 GMT+0800","2024-04-16T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Deck steel jobs to list in one separate sheet for follow up and rectification.\n\n","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","Equipment Related","11.4","Very High","","","Consolidated list sent on 22nd Apr 2024","2024-07-15T23:59:35","","Completed","2024-05-22T23:59:35","No","No","No","Internal"]
[null,null,null,35692,27004,"48_Sat Jun 01 2024 00:04:59 GMT+0800","2024-04-16T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","EGCS top three bracing forward pin worn out. Check repair and tighten.","","","Equipment Related","10.32","Very High","","","Tightened the bolts, they were loose . Lubricated with grease.","2024-06-15T23:59:35","","Completed","2024-05-31T23:59:35","No","No","No","Internal"]
[null,null,null,35322,53389,"0_Fri May 24 2024 19:33:24 GMT+0800","2024-04-16T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","BOTH LIFEBOAT STEERING CABLES TO LUBRICATE, STEERING HARD TO MOVE. INTERNAL SCRUBBING REQUIRED FOR BOTH THE BOATS","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","Greasing carried out. Steering free to move now. Both boats cleaned","2024-07-11T23:59:35","","Completed","2024-04-24T23:59:35","No","No","No","Internal","completed at the time of inspection with 3O"]
[null,null,null,35323,98032,"0_Fri May 24 2024 19:30:58 GMT+0800","2024-04-16T23:59:35","Defect,Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","COP#3 OIL LEAK FROM OIL FILLED GEAR COUPLING ABOVE TOP MECH. SEAL. LOWER SEAL MINOR LEAK TO MONITOR","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","Excess oil was drained and monitored, no leak was observed, further monitoring will be carried out during Line pressure testing and discharging operations","2024-07-15T23:59:35","","Completed","2024-05-28T23:59:35","No","No","No","Internal"]
[null,null,null,null,45937,"48_Fri May 24 2024 19:23:38 GMT+0800","2024-03-30T08:00:00","Breakdown","Ship Staff","Ship Staff Insp.","Wheel house A.C. condenser fan motor not starting","Accommodation","","Equipment Related","11.16","Low","","","Spares received at Corpus Christie and same installed and made Bridge AC operational.","2024-06-29T08:00:00","STAI 240063","Completed","2024-06-15T08:00:00","No","No","No","Internal","PO processed, awaiting spares connection"]
[null,null,null,null,36556,"48_Fri Jun 28 2024 18:36:30 GMT+0800","2024-06-11T08:00:00","Defect","Ship Staff","Ship Staff Insp.","ME unit no 2 return line from fuel injector leaking","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Rectified by replacing fittings and pipings","2024-06-21T08:00:00","","Completed","2024-06-15T08:00:00","No","No","No","Internal"]
[null,null,null,null,99788,"48_Wed Jul 03 2024 02:02:52 GMT+0800","2024-06-15T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Fixed Gas detection system of both BWT and P/P room triggers alarm every 6 hours","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","Pump room gas detection system one flow switch renewed and one solenoid was stuck same rectified.\nWater ballast tank gas detection system flow switch and vacuum switch renewed. Transport pump con rod was broken same pump renewed.\nboth the system are operational.","2024-09-25T08:00:00","","Completed","2024-07-09T08:00:00","No","No","No","Internal"]
[null,null,null,null,52776,"0_Tue Jul 02 2024 23:31:57 GMT+0800","2024-06-18T08:00:00","Observation","Ship Staff","Ship Staff Insp.","Main deck walkway few ramps found wasted ","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.8","Low","","","Dismantled and shifted to engine room workshop, hot work repairs carried out, painted and installed back","2024-07-22T08:00:00","","Completed","2024-07-06T08:00:00","No","No","No","Internal"]
[null,null,null,null,33948,"0_Tue Jul 02 2024 23:27:17 GMT+0800","2024-06-18T08:00:00","Observation","Ship Staff","Ship Staff Insp.","VRCS hydraulic box covers securing lugs & hinges found heavily rusted seared and holed","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","11.4","Very High","","","Hot work repairs completed and installed back","2024-09-18T08:00:00","","Completed","2024-06-29T08:00:00","No","No","No","Internal"]
[null,null,null,null,11603,"0_Tue Jul 02 2024 23:17:57 GMT+0800","2024-06-18T08:00:00","Observation","Ship Staff","Ship Staff Insp.","Port provision crane de rusting and painting required","Deck - Machinery","General Appearance","Equipment Related","11.8","Low","","","De rusting and painting carried out","2024-09-18T08:00:00","","Completed","2024-07-26T08:00:00","No","No","No","Internal"]
[null,null,null,null,65046,"0_Tue Jul 02 2024 23:07:17 GMT+0800","2024-06-18T08:00:00","Observation","Ship Staff","Ship Staff Insp.","Bunker tanks vents & savealls are in poor rusted condition ","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","Equipment Related","11.7","High","","","De rusted and painted","2024-09-18T08:00:00","","Completed","2024-07-20T08:00:00","No","No","No","Internal"]
[null,null,null,null,73835,"0_Tue Jul 02 2024 23:04:29 GMT+0800","2024-06-18T08:00:00","Observation","Ship Staff","Ship Staff Insp.","Rope store hatch pad lock eye wasted & sheared off ","Miscellaneous","Structural Condn. / WT integrity ","Equipment Related","11.6","Medium","","","Welded with hot work permit and concurrence","2024-09-18T08:00:00","","Completed","2024-07-16T08:00:00","No","No","No","Internal"]
[null,null,null,null,92319,"48_Mon Jul 01 2024 03:08:58 GMT+0800","2024-06-17T08:00:00","Breakdown","Ship Staff","Ship Staff Insp.","Pump room motor fan davit has big hole","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","Equipment Related","11.4","Very High","","","Davit dismantled, shifted to engine room, hot work repairs and painting carried out","2024-08-17T08:00:00","","Completed","2024-06-30T08:00:00","No","No","No","Internal"]
[null,null,null,null,17971,"48_Tue Jul 02 2024 23:01:20 GMT+0800","2024-06-18T08:00:00","Observation","Ship Staff","Ship Staff Insp.","Port and stbd provision crane hose securing lugs supports have broken down ","Deck - Machinery","General Appearance","Equipment Related","10.28","Low","","","Rectified after taking hot work concurrence from office","2024-09-18T08:00:00","","Completed","2024-07-17T08:00:00","No","No","No","Internal"]
[null,null,null,null,16867,"0_Mon Jul 01 2024 03:12:49 GMT+0800","2024-04-22T08:00:00","Breakdown","Ship Staff","Ship Staff Insp.","Light fittings on sunken deck and beneath the scrubber tower supporting\nplates wasted","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.11","Very High","","","Hot work concurrence obtained and renewed, installation of light in progress","2024-07-21T08:00:00","","Completed",null,"No","No","No","Internal"]
[null,null,null,null,92703,"0_Mon Jul 01 2024 03:25:14 GMT+0800","2024-06-18T08:00:00","Observation","Ship Staff","Ship Staff Insp.","Sunken Deck Sound reception system Back supporting plate wasted,","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.35","Medium","","","Renewed ","2024-08-18T08:00:00","","Completed","2024-07-16T08:00:00","No","No","No","Internal"]
[null,null,null,null,21636,"0_Tue Jul 02 2024 23:23:46 GMT+0800","2024-06-18T08:00:00","Observation","Ship Staff","Ship Staff Insp.","Accommodation superstructure side, aft bulkheads, ER Funnel casing and scrubber tower is in poor state and require extensive de-rusting and painting ","Accommodation","General Appearance","Equipment Related","11.8","Low","","","De-rusting and spot painting carried out","2024-09-18T08:00:00","","Completed","2024-07-20T08:00:00","No","No","No","Internal"]
[null,null,null,null,96691,"48_Tue Jul 02 2024 05:06:21 GMT+0800","2024-06-21T08:00:00","Defect","Ship Staff","Ship Staff Insp.","ETO reported 220 volt Low insulation made to infinity in wrong way. Wires are swapped","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Low insulation rectified and wires connected properly.","2024-09-26T08:00:00","","Completed","2024-07-16T08:00:00","No","No","No","Internal"]
[null,null,null,null,70325,"48_Tue Jul 02 2024 05:04:44 GMT+0800","2024-06-19T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Incinerator waste oil  pump seal is leaking and hence they are not burning sludge","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Lip seal replaced and spare ordered ","2024-09-26T08:00:00","","Completed","2024-07-02T08:00:00","No","No","No","Internal"]
[null,null,null,null,43050,"48_Tue Jul 02 2024 04:32:17 GMT+0800","2024-06-20T08:00:00","Defect","Ship Staff","Ship Staff Insp.","DG exhaust gas leaks from manifold need to inspect expansion bellows","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Exhuast piping gasket and bellow was replaced","2024-09-12T08:00:00","","Completed","2024-07-17T08:00:00","No","No","No","Internal"]
[null,null,null,null,58322,"48_Tue Jul 02 2024 04:28:57 GMT+0800","2024-06-27T08:00:00","Defect","Ship Staff","Ship Staff Insp.","M/E waste Gate solenoid valve is faulty and same needs replacement","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Spare valve ready and same replaced on 28/07/2024","2024-09-05T08:00:00","","Completed","2024-07-28T08:00:00","No","No","No","Internal"]
[null,null,null,null,49156,"0_Mon Jul 01 2024 03:16:11 GMT+0800","2024-06-18T08:00:00","Observation","Ship Staff","Ship Staff Insp.","Many light fittings & their securing plate stub pieces around the\naccommodation, P/R block & funnel casing found heavily rusted. ","Miscellaneous","General Appearance","External Factors","11.10","Medium","","","De-rusting, 1st and 2nd coat painting work completed, Final coat painting done lights fitted back in position","2024-08-18T08:00:00","","Completed","2024-07-25T08:00:00","No","No","No","Internal"]
[null,null,null,null,21728,"48_Sat Jun 01 2024 00:26:08 GMT+0800","2024-04-16T08:00:00","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","WHRS exh leak to identify and take corrective action.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Leak rectified.","2024-07-15T08:00:00","","Completed","2024-06-09T08:00:00","No","No","No","Internal","Awaiting suitable opportunity for the job, planned at Corpus as per time available"]
[null,null,null,null,11981,"48_Tue Jul 02 2024 04:34:03 GMT+0800","2024-06-07T08:00:00","Defect","Ship Staff","Ship Staff Insp.","WHRS Inspection door gland packing hardened and needs to be replaced","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","WHRS door leak rectified,","2024-09-05T08:00:00","STAI240176","Completed","2024-06-09T08:00:00","No","No","No","Internal"]
[null,null,null,null,84827,"48_Wed Jul 03 2024 01:58:10 GMT+0800","2024-06-15T08:00:00","Defect","Ship Staff","Ship Staff Insp.","SAAB COT 5 CENTRE NO ULLAGE READING","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","Spare received, renewed and made operational.","2024-09-18T08:00:00","STAI 240173","Completed",null,"No","No","No","Internal"]

{"sheet":"Calc","index":2,"n_rows":28,"n_cols":12,"rows_kept":28,"cut":false,"hidden":true,"merged":[]}
["Def_type","Def_cause","Equipments","VIQrefno","Observer_code"]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,"Dim itemSele As Long"]
[null,null,null,null,null,null,null,null,null,null,null,"   dim startRow as integer"]
[null,null,null,null,null,null,null,null,null,null,null,"   startRow=1"]
[null,null,null,null,null,null,null,null,null,null,null,"        For itemSele = 0 To ListBox1.ListCount - 1"]
[null,null,null,null,null,null,null,null,null,null,null,"        If ListBox1.Selected(itemSele) = True Then"]
[null,null,null,null,null,null,null,null,null,null,null,"        Worksheets(\"WorksheetName\").Range(\"A\" & startRow).Value = ListBox1.List(itemSele)"]
[null,null,null,null,null,null,null,null,null,null,null,"        startRow = startRow + 1"]
[null,null,null,null,null,null,null,null,null,null,null,"        End If"]
[null,null,null,null,null,null,null,null,null,null,null,"        Next"]
[null,null,null,null,null,null,null,null,null,null,null,"Dim LastRowA As String"]
[null,null,null,null,null,null,null,null,null,null,null,"        Dim itemSele As Long"]
[null,null,null,null,null,null,null,null,null,null,null,"       Dim startRow as integer"]
[null,null,null,null,null,null,null,null,null,null,null,"        LastRowA = ActiveSheet.Cells(Rows.count, \"A\").End(xlUp).row"]
[null,null,null,null,null,null,null,null,null,null,null,"        startQue = 0"]
[null,null,null,null,null,null,null,null,null,null,null,"        For itemSele = 0 To ListBox1.ListCount - 1"]
[null,null,null,null,null,null,null,null,null,null,null,"        For startRow = 1 To LastRowA"]
[null,null,null,null,null,null,null,null,null,null,null,"        If Worksheets(\"WorksheetName\").Range(\"A\" & startRow).Value = ListBox1.List(itemSele) Then"]
[null,null,null,null,null,null,null,null,null,null,null,"        ListBox1.Selected(itemSele) = True"]
[null,null,null,null,null,null,null,null,null,null,null,"        Exit For"]
[null,null,null,null,null,null,null,null,null,null,null,"        End If"]
[null,null,null,null,null,null,null,null,null,null,null,"        Next j"]
[null,null,null,null,null,null,null,null,null,null,null,"        Next"]
[null,null,null,null,null,null,null,null,null,null,null,"        End If"]

{"sheet":"Areaofobs","index":3,"n_rows":17,"n_cols":2,"rows_kept":17,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Cargo / Ballast Systems",11]
["Cert. & Docu.",2]
["Communication",6]
["Crew Management",3]
["Emgcy. Systems",13]
["Eng. / Strg. Comp.",14]
["General Appearance",15]
["Ice Opns.",17]
["ISM Related",7]
["ISPS Related",10]
["MARPOL Related",9]
["MLC Related",4]
["Mooring",12]
["Navigation",5]
["Safety / LSA / FFA",8]
["Structural Condn. / WT integrity ",16]

{"sheet":"Vessel_type","index":4,"n_rows":1,"n_cols":2,"rows_kept":1,"cut":false,"hidden":true,"merged":[]}
["Vessel_type","ID"]

{"sheet":"Deficiency_type","index":5,"n_rows":8,"n_cols":3,"rows_kept":8,"cut":false,"hidden":true,"merged":[]}
["TITLE","Type of deficiency_description","ID"]
["Breakdown",null,6]
["Critical Equipment",null,4]
["Defect",null,1]
["Guarantee Claim",null,8]
["Non Conformity",null,2]
["Observation",null,3]
["Other",null,7]

{"sheet":"VIQrefno","index":6,"n_rows":427,"n_cols":3,"rows_kept":427,"cut":false,"hidden":true,"merged":[]}
["VIQ_ref_no","Risk Value of observation","ID"]
["1.1","Low",8243]
["1.10","Low",8252]
["1.11","Low",8253]
["1.12","Low",8254]
["1.13","Low",8255]
["1.14","Low",8256]
["1.15","Low",8257]
["1.16","Low",8259]
["1.17","Low",8260]
["1.18","Low",8261]
["1.19","Low",8262]
["1.2","Low",8244]
["1.20","Low",8263]
["1.21","Low",8265]
["1.22","Low",8266]
["1.23","Low",8267]
["1.24","Low",8268]
["1.25","Low",8269]
["1.26","Low",8270]
["1.3","Low",8245]
["1.4","Low",8246]
["1.5","Low",8247]
["1.6","Low",8248]
["1.7","Low",8249]
["1.8","Low",8250]
["1.9","Low",8251]
["1.99","High",11258]
["10.1","Medium",8461]
["10.10","High",8470]
["10.11","Medium",8471]
["10.12","Very High",8472]
["10.13","Very High",8473]
["10.14","Medium",8474]
["10.15","Low",8475]
["10.16","Very High",8476]
["10.17","Very High",8477]
["10.18","High",8478]
["10.19","Very High",8479]
["10.2","Low",8462]
["10.20","High",8480]
["10.21","Medium",8481]
["10.22","Low",8482]
["10.23","Medium",8483]
["10.24","Low",8484]
["10.25","Very High",8485]
["10.26","High",8486]
["10.27","Medium",8487]
["10.28","Low",8488]
["10.29","Medium",8489]
["10.3","Medium",8463]
["10.30","High",8490]
["10.31","Very High",8491]
["10.32","Very High",8492]
["10.33","High",8493]
["10.34","High",8494]
["10.35","Very High",8495]
["10.36","Very High",8496]
["10.37","Medium",8497]
["10.38","Medium",8498]
["10.39","High",8499]
["10.4","High",8464]
["10.40","Medium",8500]
["10.41","Medium",8501]
["10.42","Medium",8502]
["10.43","Medium",8503]
["10.44","Medium",8504]
["10.45","Very High",8505]
["10.46","High",8506]
["10.47","Medium",8507]
["10.48","High",8508]
["10.49","Medium",8509]
["10.5","Low",8465]
["10.50","High",8510]
["10.51","Low",8511]
["10.52","Medium",8512]
["10.53","Medium",8513]
["10.54","High",8514]
["10.55","Low",8515]
["10.6","Very High",8466]
["10.7","Medium",8467]
["10.8","Medium",8468]
["10.9","Medium",8469]
["10.99","High",8516]
["11.1","High",8420]
["11.10","Medium",8429]
["11.11","Very High",8430]
["11.12","Low",8431]
["11.13","Low",8432]
["11.14","Medium",8433]
["11.15","Low",8434]
["11.16","Low",8435]
["11.17","Low",8436]
["11.2","Medium",8421]
["11.3","Medium",8422]
["11.4","Very High",8423]
["11.5","Medium",8424]
["11.6","Medium",8425]
["11.7","High",8426]
["11.8","Low",8427]
["11.9","Low",8428]
["11.99","High",8437]
["12.1","High",8438]
["12.10","High",8448]
["12.11","High",8449]
["12.12","High",8450]
["12.13","High",8451]
["12.14","High",8452]
["12.15","High",8453]
["12.16","High",8454]
["12.17","High",8455]
["12.18","High",8456]
["12.19","High",8457]
["12.2","High",8439]
["12.20","High",8458]
["12.21","High",8459]
["12.3","High",8441]
["12.4","High",8442]
["12.5","High",8443]
["12.6","High",8444]
["12.7","High",8445]
["12.8","High",8446]
["12.9","High",8447]
["12.99","High",8460]
["2.1","Very High",8296]
["2.1.9","Very High",11259]
["2.10","Medium",8304]
["2.11","Medium",8305]
["2.12","Low",8306]
["2.13","Low",8307]
["2.14","Low",8308]
["2.15","Low",8309]
["2.16","Medium",8310]
["2.2","Medium",8297]
["2.3","High",8295]
["2.4","Medium",8298]
["2.5","Medium",8299]
["2.6","Low",8300]
["2.7","High",8301]
["2.8","High",8302]
["2.9","Medium",8303]
["2.99","High",8311]
["3.1","High",8312]
["3.2","Very High",8313]
["3.3","High",8314]
["3.4","Low",8294]
["3.5","Medium",8315]
["3.6","High",8316]
["3.7","Very High",8317]
["3.8","Very High",8318]
["3.99","High",8319]
["4.1","High",8320]
["4.10","High",8329]
["4.11","Medium",8330]
["4.12","Very High",8331]
["4.13","Very High",8332]
["4.14","Very High",8333]
["4.15","Very High",8334]
["4.16","Very High",8335]
["4.17","Very High",8336]
["4.18","Very High",8337]
["4.19","Low",8338]
["4.2","Medium",8321]
["4.20","Very High",8339]
["4.21","High",8340]
["4.22","Low",8341]
["4.23","High",8342]
["4.24","High",8343]
["4.25","Low",8344]
["4.26","Low",8345]
["4.27","High",8346]
["4.3","Medium",8322]
["4.4","High",8323]
["4.5","Very High",8324]
["4.6","Medium",8325]
["4.7","High",8326]
["4.8","Medium",8327]
["4.9","Medium",8328]
["4.99","High",8347]
["5.1","Very High",8517]
["5.10","High",8526]
["5.11","Low",8527]
["5.12","Medium",8528]
["5.13","High",8529]
["5.14","Very High",8530]
["5.15","Medium",8531]
["5.16","Very High",8532]
["5.17","Very High",8533]
["5.18","High",8534]
["5.19","Medium",8535]
["5.2","Very High",8518]
["5.20","Medium",8536]
["5.21","Medium",8537]
["5.22","High",8539]
["5.23","Very High",8540]
["5.24","Very High",8541]
["5.25","Medium",8542]
["5.26","Medium",8543]
["5.27","Medium",8544]
["5.28","Very High",8545]
["5.29","High",8546]
["5.3","Low",8519]
["5.30","High",8547]
["5.31","High",8548]
["5.32","High",8549]
["5.33","High",8550]
["5.34","Low",8551]
["5.35","Medium",8552]
["5.36","Low",8553]
["5.37","Low",8554]
["5.38","High",8555]
["5.39","Very High",8556]
["5.4","High",8520]
["5.40","Very High",8557]
["5.41","Very High",8558]
["5.42","Medium",8559]
["5.43","High",8560]
["5.44","High",8561]
["5.45","Medium",8564]
["5.46","Medium",8565]
["5.47","Medium",8566]
["5.48","Medium",8567]
["5.5","Low",8521]
["5.6","Low",8522]
["5.7","Medium",8523]
["5.8","Medium",8524]
["5.9","Very High",8525]
["5.99","High",8568]
["6.1","Medium",8348]
["6.10","Low",8357]
["6.11","High",8358]
["6.12","Medium",8359]
["6.13","Low",8360]
["6.14","High",8361]
["6.15","High",8362]
["6.16","Very High",8363]
["6.17","Very High",8364]
["6.18","Medium",8365]
["6.19","Low",8366]
["6.2","High",8349]
["6.20","Medium",8367]
["6.21","High",8368]
["6.22","Medium",8369]
["6.3","Low",8350]
["6.4","High",8351]
["6.5","Medium",8352]
["6.6","Medium",8353]
["6.7","High",8354]
["6.8","High",8355]
["6.9","Low",8356]
["6.99","High",8370]
["7.1","High",8371]
["7.10","High",8380]
["7.11","High",8381]
["7.12","High",8382]
["7.13","Medium",8383]
["7.14","Medium",8384]
["7.15","High",8385]
["7.16","High",8386]
["7.17","High",8387]
["7.2","High",8372]
["7.3","Low",8373]
["7.4","Low",8374]
["7.5","Low",8375]
["7.6","Medium",8376]
["7.7","Low",8377]
["7.8","High",8378]
["7.9","High",8379]
["7.99","High",8388]
["8.1","Very High",8569]
["8.10","Very High",8578]
["8.100","Low",11227]
["8.101","Medium",11228]
["8.102","Low",11229]
["8.103","Low",11230]
["8.104","Low",11231]
["8.105","Medium",11232]
["8.106","Medium",11233]
["8.107","Low",11234]
["8.108","High",11235]
["8.109","Very High",11236]
["8.11","Medium",8579]
["8.110","High",11237]
["8.111","Medium",11238]
["8.112","High",11239]
["8.113","Medium",11240]
["8.114","Low",11241]
["8.115","High",11242]
["8.116","Medium",11243]
["8.117","Medium",11244]
["8.118","Medium",11245]
["8.119","High",11246]
["8.12","Medium",8580]
["8.120","High",11247]
["8.121","Medium",11248]
["8.122","High",11249]
["8.123","High",11250]
["8.124","Low",11251]
["8.125","High",11252]
["8.126","Medium",11253]
["8.127","Medium",11254]
["8.13","Medium",8581]
["8.14","Very High",8582]
["8.15","High",8583]
["8.16","Very High",8584]
["8.17","Low",8585]
["8.18","High",8586]
["8.19","High",8587]
["8.199","High",11255]
["8.2","Medium",8570]
["8.20","Medium",8588]
["8.21","High",8589]
["8.22","Very High",8590]
["8.23","Medium",8591]
["8.24","Medium",8592]
["8.25","Very High",8593]
["8.26","High",8594]
["8.27","Medium",8595]
["8.28","Medium",8596]
["8.29","High",8598]
["8.3","Very High",8571]
["8.30","High",8599]
["8.31","High",8600]
["8.32","Low",8601]
["8.33","Medium",8602]
["8.34","High",8603]
["8.35","Medium",8604]
["8.36","Medium",8605]
["8.37","High",8607]
["8.38","Medium",8608]
["8.39","Medium",8609]
["8.4","Medium",8572]
["8.40","High",8610]
["8.41","Medium",8611]
["8.42","Medium",8612]
["8.43","Very High",8613]
["8.44","High",8615]
["8.45","High",8616]
["8.46","Very High",8617]
["8.47","Very High",8618]
["8.48","Medium",8619]
["8.49","High",8620]
["8.5","Very High",8573]
["8.50","Medium",8621]
["8.51","Low",8622]
["8.52","Low",8623]
["8.53","Low",8624]
["8.54","High",8625]
["8.55","Low",11182]
["8.56","Medium",11183]
["8.57","Medium",11184]
["8.58","High",11185]
["8.59","High",11186]
["8.6","Medium",8574]
["8.60","High",11187]
["8.61","Medium",11188]
["8.62","Very High",11189]
["8.63","High",11190]
["8.64","Medium",11191]
["8.65","Low",11192]
["8.66","High",11193]
["8.67","High",11194]
["8.68","High",11195]
["8.69","Medium",11196]
["8.7","High",8575]
["8.70","Medium",11197]
["8.71","Very High",11198]
["8.72","Medium",11199]
["8.73","Medium",11200]
["8.74","High",11201]
["8.75","Medium",11202]
["8.76","Medium",11203]
["8.77","Medium",11204]
["8.78","Medium",11205]
["8.79","Medium",11206]
["8.8","Medium",8576]
["8.80","Medium",11207]
["8.81","Low",11208]
["8.82","Medium",11209]
["8.83","Low",11210]
["8.84","Low",11211]
["8.85","Medium",11212]
["8.86","Medium",11213]
["8.87","Medium",11214]
["8.88","Low",11215]
["8.89","High",11216]
["8.9","High",8577]
["8.90","High",11217]
["8.91","High",11218]
["8.92","Medium",11219]
["8.93","Low",11220]
["8.94","Low",11221]
["8.95","Medium",11222]
["8.96","Medium",11223]
["8.97","Low",11224]
["8.98","High",11225]
["8.99","Medium",11226]
["9.1","Low",8390]
["9.10","Medium",8399]
["9.11","Medium",8400]
["9.12","Medium",8401]
["9.13","Low",8402]
["9.14","Medium",8403]
["9.15","Medium",8404]
["9.16","High",8405]
["9.17","High",8406]
["9.18","Low",8407]
["9.19","Low",8408]
["9.2","Very High",8391]
["9.20","Medium",8409]
["9.21","Medium",8410]
["9.22","Low",8411]
["9.23","Low",8412]
["9.24","Medium",8413]
["9.25","Low",8414]
["9.26","Low",8415]
["9.27","Low",8416]
["9.28","Medium",8417]
["9.29","Low",8418]
["9.3","Very High",8392]
["9.4","High",8393]
["9.5","High",8394]
["9.6","Low",8395]
["9.7","Medium",8396]
["9.8","Medium",8397]
["9.9","Medium",8398]
["9.99","High",8419]

{"sheet":"Equipment_list","index":7,"n_rows":28,"n_cols":3,"rows_kept":28,"cut":false,"hidden":true,"merged":[]}
["TITLE","Equipment_list_description","ID"]
["Accommodation",null,12]
["Cargo Mach.",null,13]
["Critical Equip.",null,16]
["Deck - Machinery",null,18]
["Deck - Mooring Machinery",null,15]
["Deck - Pipe / Fittings",null,20]
["Documentation",null,21]
["E/R - Air Comp.",null,8]
["E/R - Aux. Engine",null,4]
["E/R - Aux. Mach.",null,7]
["E/R - Boiler",null,5]
["E/R - Main Engine",null,3]
["E/R - Pipes/ valves & fittings",null,9]
["E/R - Pumps",null,32]
["E/R - Purifier",null,6]
["Elect. Mach. & Equip.",null,10]
["Hull & Tanks",null,19]
["Inert Gas",null,14]
["LSA / FFA",null,17]
["Miscellaneous",null,22]
["Navigation - DGPS / EPFS / AIS",null,28]
["Navigation - ECDIS",null,25]
["Navigation - Echo Sounder / Speed Log",null,26]
["Navigation - GMDSS & Communication",null,23]
["Navigation - Others",null,11]
["Navigation - RADAR",null,24]
["Navigation - VDR / BNWAS",null,30]

{"sheet":"PSC_MOU","index":8,"n_rows":11,"n_cols":3,"rows_kept":11,"cut":false,"hidden":true,"merged":[]}
["TITLE","PSC_MOU_description","ID"]
["Asia and the Pacific",null,2]
["Caribbean",null,4]
["Europe and the North Atlantic",null,1]
["Latin America",null,3]
["The Black Sea region",null,6]
["The Indian Ocean",null,8]
["The Mediterranean",null,7]
["The Riyadh MoU",null,9]
["USCG",null,10]
["West and Central Africa",null,5]

{"sheet":"Inspection_type","index":9,"n_rows":13,"n_cols":2,"rows_kept":13,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Bunkering Audit",14]
["Cargo Audit",17]
["Engineering Audit",16]
["ISM Audit",2]
["ISPS Audit",3]
["IT Audit",10]
["MLC Audit",1]
["Mooring Audit",9]
["Nav Audit / Verification",8]
["Onboard Training",18]
["Ship Staff Insp.",15]
["Suptd. Insp.",13]

{"sheet":"Deficiency_Cause","index":10,"n_rows":8,"n_cols":3,"rows_kept":8,"cut":false,"hidden":true,"merged":[]}
["TITLE","Deficiency_Cause_description","ID"]
["Behaviour Based",null,1]
["Equipment Related",null,4]
["External Factors",null,5]
["Human Error",null,7]
["Inappropriate Procedure",null,8]
["Industry Issue",null,6]
["Knowledge Based",null,3]

{"sheet":"Observer_code","index":11,"n_rows":3,"n_cols":3,"rows_kept":3,"cut":false,"hidden":true,"merged":[]}
["TITLE","Observer_code_description","ID"]
["Owner / Marine / Tech. Suptd.",null,3]
["Ship Staff",null,2]

{"sheet":"Status_code","index":12,"n_rows":6,"n_cols":3,"rows_kept":6,"cut":false,"hidden":true,"merged":[]}
["TITLE","Status_code_description","ID"]
["Completed",null,6]
["Deferred to D D",null,5]
["In progress",null,3]
["Not Started",null,2]
["Waiting spare",null,4]

{"sheet":"PSC_ref_no","index":13,"n_rows":19,"n_cols":2,"rows_kept":19,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Alarms",9]
["Cargo operations including equipment",7]
["Certificates & Documentation",2]
["Dangerous Goods",13]
["Emergency Systems",5]
["Fire safety",8]
["ISM",16]
["ISPS",17]
["Life saving appliances",12]
["MLC, 2006",18]
["Other",19]
["Pollution Prevention",15]
["Propulsion and auxiliary machinery",14]
["Radio communication",6]
["Safety of Navigation",11]
["Structural condition",3]
["Water/Weathertight condition",4]
["Working and Living Conditions",10]

{"sheet":"Risk_value_of_obs","index":14,"n_rows":1,"n_cols":2,"rows_kept":1,"cut":false,"hidden":true,"merged":[]}
["Risk Value of observation","ID"]

{"sheet":"Year","index":15,"n_rows":18,"n_cols":1,"rows_kept":18,"cut":false,"hidden":true,"merged":[]}
["Year"]
[2014]
[2015]
[2016]
[2017]
[2018]
[2019]
[2020]
[2021]
[2022]
[2023]
[2024]
[2025]
[2026]
[2027]
[2028]
[2029]
[2030]

{"sheet":"Month","index":16,"n_rows":13,"n_cols":1,"rows_kept":13,"cut":false,"hidden":true,"merged":[]}
["Month"]
["Jan"]
["Feb"]
["Mar"]
["Apr"]
["May"]
["Jun"]
["Jul"]
["Aug"]
["Sep"]
["Oct"]
["Nov"]
["Dec"]

{"sheet":"Date_","index":17,"n_rows":32,"n_cols":1,"rows_kept":32,"cut":false,"hidden":true,"merged":[]}
["Date"]
["01"]
["02"]
["03"]
["04"]
["05"]
["06"]
["07"]
["08"]
["09"]
[10]
[11]
[12]
[13]
[14]
[15]
[16]
[17]
[18]
[19]
[20]
[21]
[22]
[23]
[24]
[25]
[26]
[27]
[28]
[29]
[30]
[31]

{"sheet":"Sheet1","index":18,"n_rows":24,"n_cols":6,"rows_kept":24,"cut":false,"hidden":true,"merged":[]}
[]
[null,"ID","E",null,"Date Recorded",1]
[null,"UNIQUE ID","F",null,"Type of Deficiency",2]
[1,"Date Recorded","G",null,"Observer code",3]
["ignore","Vessel Type","H",null,"Type of Inspection",4]
[null,"Internal / External","I",null,"Description of Deficiency",5]
[null,"Drydock","J",null,"Equipment Categories",6]
[null,"Information Sharing","K",null,"Area of Observation",7]
[null,"Critical_item","L",null,"Deficiency Cause",8]
[null,"Deficiency Type","M",null,"VIQ Ref Number",9]
[null,"Deficiency Cause","N",null,"Risk Value of Obs",10]
[null,"Inspection Type","O",null,"PSC Ref Number",11]
[null,"Equipments","P",null,"PSC MOU ID",12]
[null,"VIQ Reference Number","Q",null,"Action Taken or Required",13]
[null,"Risk Value of the observation","R",null,"Target Date",14]
[null,"PSC Reference Number","S",null,"PO Ref No.",15]
[null,"PSC MOU","T",null,"Status Code",16]
[null,"Observer Code","U",null,"Date Completed",17]
[null,"Target Date","V",null,"Drydock",18]
[null,"Status Code","W",null,"Info Sharing",19]
[null,"Description of Deficiency","X",null,"Critical Item Flag",20]
[null,"Action taken / required","Y",null,"Audit Type",21]
[null,"PO ref no","Z"]
[null,"Date completed","AA"]

{"sheet":"Ship_information","index":19,"n_rows":2,"n_cols":4,"rows_kept":2,"cut":false,"hidden":true,"merged":[]}
["Ship_ID","Ship_Name","FILE_NAME","Export_Date"]
["48","DHT TAIGA (01-06-2024)","48_1717222351214.xlsm","2024-07-30 23:07:15"]

{"sheet":"External_Deficiency_type","index":20,"n_rows":5,"n_cols":3,"rows_kept":5,"cut":false,"hidden":true,"merged":[]}
["TITLE","Type of deficiency_description","ID"]
["Condn of Class / Memo",null,5]
["Defect",null,1]
["Non Conformity",null,2]
["Observation",null,3]

{"sheet":"External_Inspection_type","index":21,"n_rows":11,"n_cols":2,"rows_kept":11,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Cargo Audit",17]
["Flag State Insp.",5]
["ISM Audit",2]
["ISPS Audit",3]
["MLC Audit",1]
["Nav Audit / Verification",8]
["OM Insp. (Eg. SIRE / CDI etc.)",6]
["Others (Eg. Insurance etc.)",12]
["PSC Inspection",4]
["Terminal Insp.",11]

{"sheet":"External_Observer_code","index":22,"n_rows":7,"n_cols":3,"rows_kept":7,"cut":false,"hidden":true,"merged":[]}
["TITLE","Observer_code_description","ID"]
["Class Surveyor",null,4]
["FSC Inspector",null,5]
["Others (Eg. Insurance etc.)",null,9]
["PSC Insp.",null,6]
["SIRE / CDI Insp.",null,8]
["Terminal Insp.",null,7]

{"sheet":"Sheet Version","index":23,"n_rows":2,"n_cols":2,"rows_kept":2,"cut":false,"hidden":true,"merged":[]}
["Version","Title"]
["2.0","Version 2.0"]