{"text_format":"1","workbook":"xlsx","n_sheets":24,"sheets":["Mainsheet","Completed","Calc","Areaofobs","Vessel_type","Deficiency_type","VIQrefno","Equipment_list","PSC_MOU","Inspection_type","Deficiency_Cause","Observer_code","Status_code","PSC_ref_no","Risk_value_of_obs","Year","Month","Date_","Sheet1","Ship_information","External_Deficiency_type","External_Inspection_type","External_Observer_code","Sheet Version"],"not_rendered":{"charts":0,"images":1,"macros":1,"external_links":0,"defined_names":12,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Mainsheet","index":0,"n_rows":37,"n_cols":28,"rows_kept":37,"cut":false,"hidden":false,"merged":[[10,8,10,9],[10,12,10,13],[12,6,12,27],[8,6,8,27]]}
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,"Defect - Damage Monitoring Sheet"]
[]
[null,null,null,null,null,null,null,"Date of Report","06-Aug-2024",null,null,"Ship Name","DHT BAUHINIA (22-07-2024)"]
[]
[null,null,null,null,null,null,"VERSION : 2.0"]
[]
[]
[]
[null,null,null,"ID","SHIPSIDE UNIQUEID","UNIQUE ID","Date Recorded","Type of Deficiency","Observer code","Type of Inspection","Description of Deficiency","Equipment Categories","Area of Observation","Deficiency Cause","VIQ Ref Number","Risk Value of Obs","PSC Ref Number","PSC MOU ID","Action Taken or Required","Target Date","PO Ref No.","Status Code","Date Completed","Drydock","Info Sharing","Critical Item","Audit Type","Superintendent Remarks"]
[null,null,null,36210,16324,"24_Sat Jun 15 2024 13:21:02 GMT+0800","2024-05-29T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Boiler control panel unit cooler faulty. Flicker Stop and Alarm Reset push button switches covers broken. ","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Hermetic compressor found faulty, unit cooler is presently operating in fan mode only. Unit cooler to be renewed.  Push buttons to be renewed. RO raised.","2024-08-29T23:59:35","DBAU240151","Waiting spare",null,"No","No","No","Internal"]
[null,null,null,36209,78817,"24_Sat Jun 15 2024 21:09:27 GMT+0800","2024-05-30T23:59:35","Defect,Observation","Ship Staff","Ship Staff Insp.","1P, 2P, 3P, FPK, APK Ballast tank Remote sounding gauge erratic","Elect. Mach. & Equip.","Cargo / Ballast Systems","Equipment Related","8.13","Medium","","","1P, 2P, 2S,3S, FPK, ballast tanks inspected. All deck lines and lines inside tanks been blown through with compress air and water. All clogging cleared. Pressure transmitter/safety chamber tested and found in working condition. Tanks sounding to be tested during Ballast operation. APK tank remote gauging lines to be blown through and tested during tank inspection. All tanks level gauges calibrated after all lines cleared and pressure transmitter/safety chamber testing completed. Gauges still not operational after servicing in drydock, have sent msg regarding the same to superintendent. Awaiting response. 1. We have checked free passage of the air line by water blowing, followed by air blowing the line, Caliberated the Zero and Span setting by pressure caliberator as per procedure in manual and size of the tank. 2. Observed the Draft gauges to show accurate, 3. 3S,4 & 5 Ballast tanks reading are working satisfactory, 4. 2P Tank was working satisfactory but presently showing full reading due to blockage of line from deck to the tank, To clear the same at convenient opportunity, 5. 1P, 2S Air lines were blanked on top of the ballast tank and observed the reading to show full in the tank indicator, The lines are leaking inside the tank hence shows empty/Partial, 6. FP, APT, 3P ballast tank Air line from the upper deck to Tank top is leaking, to identify the leak and rectify, 7. 1S Ballast tank is found to have mild leakage due to which the level does not show beyond 25M, To check for mild leak and rectify. 8. Futher investigation to be carried out during load passage as ballast tanks will be empty. All lines, pressure transmitter checked for integrity and proper working. Dead sounding for the ballast tanks calibrated. Will check during ballasting operation at discharge port. Gauges still not operational after servicing in drydock, upon troubleshooting it was found various modulators are faulty and needs replacement.","2024-08-05T23:59:35","","In progress",null,"No","No","No","Internal"]
[null,null,null,36212,15380,"24_Sat Jun 15 2024 21:36:31 GMT+0800","2024-05-30T23:59:35","Observation","Ship Staff","Ship Staff Insp.","220V low Insulation","Elect. Mach. & Equip.","General Appearance","Equipment Related","10.38","Medium","","","Please note that vessels IR monitor for 220V main supply is reading 2Mohm even when deck lights are off\nUpon inspection it was found all breakers for the lighting supply in accommodation from 220V feeder panel is having low insulation issue.\nIntermittently vessel has observed insulation resistance drops to 0.7M?.\nTroubleshooting carried out on the same and found that low insulation is occurring from accommodation lighting.\nvessel has inspected random lights in mess room, galley, alleyway hospital etc. and found all the lights supplied from main 220V has this issue resulting in low insulation.\nWires are completely destroyed and needed replacement/repairing.\nVessel also checked few lights in E/R but the cable condition was OK.\nSo far vessel has repaired Gym room (6 nos.) Crew mess room (4 nos.) CCR (3 nos) and Hospital (2 nos) and planning to repair all the lights cable gradually.\nPlease note at least 3 to 4 hour is required to repair one light, as the adjacent ceiling panel also to be opened for accessing the secured cables,  and the time will increase depending on the number of cables entering the fitting.\nThere are around 270 light fittings which requires attention and repair.\n\tWhile installing JB in the ceiling, it is a challenge to fix the J/B as the access is minimal.\nRequired material for repair has been received. Job is on hand and shall be completed on priority.","2024-08-30T23:59:35","DBAU240160","In progress",null,"No","No","No","Internal"]
[null,null,null,36219,57904,"24_Tue Jun 25 2024 17:36:05 GMT+0800","2024-06-13T23:59:35","Observation","Ship Staff","Ship Staff Insp.","3 Nos of hot plate in galley found to have insulation less than 3Mohms","Accommodation","General Appearance","Equipment Related","10.38","Medium","","","Defective hot plates to be renewed, spare hotplate onboard are not compatible. RO raised for the same.","2024-08-12T23:59:35","DBAU240154","Waiting spare",null,"No","No","No","Internal"]
[null,null,null,36217,15964,"24_Thu Jun 27 2024 19:54:50 GMT+0800","2024-06-14T23:59:35","Observation","Ship Staff","Ship Staff Insp.","No.1 BWTS Filter showing fault","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","At present BWTS No.1 filter is being flushed whenever it is being used and same to be rectified at the earliest.","2024-09-13T23:59:35","","In progress",null,"No","No","No","Internal"]
[null,null,null,24481,null,"24_16/03/2022 1:42:50 PM","2024-06-14T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Aux. Boiler #1 & #2 Local Operating Panel Screens faded.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Same to be renewed as data not easily visible. RO raised for the same awaiting supply. Although screen is satisfactory and managable.","2024-08-15T23:59:35","DBAU240151","Waiting spare",null,"No","No","No","Internal","RFQ in place. Will supply when spare parts are available. Target date for this defect should be amended to reflect current status. RO has been raised in September 2022.\nvessel must raise fresh RO in 2024 as 2022 RO  has been cancelled"]
[null,null,null,null,47233,"24_Wed Jun 19 2024 17:15:10 GMT+0800","2024-06-19T08:00:00","Observation","Ship Staff","Ship Staff Insp.","Correction on the Fire Plan and 'Record of Safety Equipment' is to be endorsed by the Class Surveyor during the next physical attendance as per Safety Circular/S-008-2024.","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.35","Medium","","","Awaiting next physical attendance by Class surveyor to endorse the fire Plan","2024-09-19T08:00:00","","In progress",null,"No","No","No","Internal"]
[null,null,null,36221,87064,"24_Thu Jun 27 2024 16:11:22 GMT+0800","2024-06-20T23:59:35","Observation","Ship Staff","Ship Staff Insp.","PORT AND STBD RUDDER ANGLE INDICATOR BACKLIGHT AND DIMMERS NOT WORKING","Navigation - Others","Navigation","Equipment Related","4.17","Very High","","","LED ILLUMINATION PLATES NEED RENEWAL.","2024-09-19T23:59:35","DBAU240161","Waiting spare",null,"No","No","No","Internal"]
[null,null,null,36218,78256,"24_Sat Jun 22 2024 22:37:22 GMT+0800","2024-06-22T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","AUS discharge valve no.2 operation defective and pneumatic controller air leaking ","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","At present AUS discharge valve fault has been rectified and it is operational. However there is air leak in pumproom for no.2 AUS discharge valve controller, which has been temporarily stopped. RO raised.","2024-09-22T23:59:35","DBAU240157","Waiting spare",null,"No","No","No","Internal"]
[null,null,null,36222,65502,"24_Sat Jun 22 2024 22:34:17 GMT+0800","2024-06-22T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","WBT SAAB radar system wrong reading","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","At present FPK, 1P, 2P, 2S, 3S WBT are showing inaccurate readings. Vessel has overhauled dual check safety chambers for FPK, 1wings, 2wings and 3 wings WBT and pressure tested the lines and confirmed that there is no leakage in them. Vessel suspecting pneumatic modulators are faulty and RO raised for the same. RO. DBAU240152","2024-09-22T23:59:35","RO. DBAU240152","Waiting spare",null,"No","No","No","Internal"]
[null,null,null,36223,84850,"24_Sat Jun 22 2024 22:21:45 GMT+0800","2024-06-22T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","Draft gauges erratic ","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","At present forward and aft draft guages are showing accurate readings. Vessel has overhauled dual check safety chambers for all four draft guages and pressure tested the lines and confirmed that there is no leakage in them. Vessel has raised RO for pneumatic Modulators which are suspected faulty. RO. DBAU240152","2024-09-21T23:59:35","RO. DBAU240152","Waiting spare",null,"No","No","No","Internal"]
[null,null,null,36500,11985,"24_Tue Jul 16 2024 13:11:30 GMT+0800","2024-07-14T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Mast Riser steam smothering lines are not in good condition and same to be renewed.","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.20","Medium","","","Vessel has raised an R.O for the supply of steam smothering lines and same will be change, once received onboard.","2024-10-14T23:59:35","DBAU240163","Waiting spare",null,"No","No","No","Internal","All damaged pipes to be renewed on priority basis with pipes you have onboard and for rest of the items we will supply in SIngapore."]
[null,null,null,null,64200,"0_Tue Jul 16 2024 21:07:39 GMT+0800","2024-07-04T08:00:00","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Steering Gear room davit and skylight needs immediate maintenance. ","Deck - Pipe / Fittings","ISM Related","Equipment Related","11.6","Medium","","","job to be planned","2024-09-04T08:00:00","","Not Started",null,"No","No","No","Internal"]
[null,null,null,null,26431,"0_Tue Jul 16 2024 21:10:17 GMT+0800","2024-07-04T08:00:00","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Starboard manifold gratings and drip tray needs to be derusted. ","Deck - Pipe / Fittings","General Appearance","Equipment Related","6.6","Medium","","","Job will be planned & carried out","2024-09-04T08:00:00","","Not Started",null,"No","No","No","Internal"]
[null,null,null,36505,76683,"24_Wed Jul 17 2024 13:27:46 GMT+0800","2024-07-17T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Loadicator computer is only opening up one condition and no other condition is opening up.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.4","Medium","","","IT dept and makers informed regarding the same.","2024-10-16T23:59:35","","In progress",null,"No","No","No","Internal"]
[null,null,null,null,53208,"24_Fri Jul 26 2024 14:08:37 GMT+0800","2024-07-25T08:00:00","Observation","Ship Staff","Ship Staff Insp.","Fwd Fire wire reel - Pedestal bearing found with crack on the body","Deck - Mooring Machinery","Mooring","Equipment Related","9.14","Medium","","","RO raised for new bearing DBAU240172","2024-10-24T08:00:00","DBAU240172","Waiting spare",null,"No","No","No","Internal"]
[null,null,null,null,40164,"24_Sun Jul 28 2024 16:07:20 GMT+0800","2024-07-27T08:00:00","Defect,Observation","Ship Staff","Ship Staff Insp.","BWTS electrolyser injection  valve body found holed and leaking near proom entrance ","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.11","Medium","","","RO raised for new valve","2024-10-27T08:00:00","DBAU240178","Waiting spare",null,"No","No","No","Internal"]
[null,null,null,null,83149,"24_Tue Jul 30 2024 20:20:00 GMT+0800","2024-07-29T08:00:00","Defect,Observation","Ship Staff","Ship Staff Insp.","During routine inspection of 5P WBT , observed buckling on the 3rd stringer from top at approx fr no. 66 . No apparent damage found on the ship side plating . Same entered in Refman ","Hull & Tanks","Structural Condn. / WT integrity ","Equipment Related","11.1","High","","","To be rectified in next DD ","2026-01-30T08:00:00","","Deferred to D D",null,"Yes","No","No","Internal"]
[null,null,null,null,83784,"24_Tue Jul 30 2024 21:07:17 GMT+0800","2024-07-30T08:00:00","Observation,Defect","Ship Staff","Ship Staff Insp.","During routine inspection of 4S WBT , observed indentation at the third stringer platform from the top on the ship side between  frame no. 72 and 73.\n\nThe indentation area is approximately 300 mm x 250mm and buckled inwards approximately 5mm\n","Hull & Tanks","Structural Condn. / WT integrity ","Equipment Related","11.1","High","","","To be rectified in next DD ","2026-01-30T08:00:00","","Deferred to D D",null,"No","No","No","Internal"]
[null,null,null,null,98866,"24_Fri Aug 02 2024 21:04:16 GMT+0800","2024-08-02T08:00:00","Defect,Observation","Ship Staff","Ship Staff Insp.","While carrying out routine maintenance on MW 4 mooring winch, the oil filling cap was holed.","Deck - Mooring Machinery","Mooring","Equipment Related","9.14","Medium","","","Vessel will carry out temporary repairs on the same and renew the gear oil after draining the old oil.","2024-09-02T08:00:00","","Not Started",null,"No","No","No","Internal"]

{"sheet":"Completed","index":1,"n_rows":1189,"n_cols":28,"rows_kept":1189,"cut":false,"hidden":false,"merged":[[10,8,10,9],[10,12,10,13],[12,6,12,27],[8,6,8,27]]}
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,"Defect - Damage Monitoring Sheet"]
[]
[null,null,null,null,null,null,null,"Date of Report","06-Aug-2024",null,null,"Ship Name","DHT BAUHINIA (22-07-2024)"]
[]
[null,null,null,null,null,null,"VERSION : 2.0"]
[]
[]
[]
[null,null,null,"ID","SHIPSIDE UNIQUEID","UNIQUE ID","Date Recorded","Type of Deficiency","Observer code","Type of Inspection","Description of Deficiency","Equipment Categories","Area of Observation","Deficiency Cause","VIQ Ref Number","Risk Value of Obs","PSC Ref Number","PSC MOU ID","Action Taken or Required","Target Date","PO Ref No.","Status Code","Date Completed","Drydock","Info Sharing","Critical Item","Audit Type","Superintendent Remarks"]
[null,null,null,29566,62873,"24_Sun Mar 26 2023 18:43:05 GMT+0800",null,"Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Torn lagging near Valve ‘OMO30 – M/E FO Inlet valve’.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Behaviour Based","10.19","Very High","","","lagging renewed.","2023-03-22T23:59:35","","Completed","2023-03-20T23:59:35","No","No","No","Internal"]
[null,null,null,9567,null,"24_07/01/2020 1:30:36 PM","2017-10-08T23:59:35","Non Conformity","Ship Staff","Ship Staff Insp.","During routine maintenance it was observed one of the  garbage drum at garbage station was not marked with dedicated category of garbage.","Miscellaneous","MARPOL Related","Human Error","6.2","High","","","Garbage drum was stencilied for dedicated category of garbage.","2019-11-08T23:59:35","","Completed","2019-10-08T23:59:35","No","No","No","Internal"]
[null,null,null,4410,null,"24_24/10/2019 11:29:27 AM","2018-12-24T23:59:35","Defect","Ship Staff","Ship Staff Insp.","2S PV Valve leaks from pressure side.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.21","High","","","Replaced with overhauled spare.","2019-01-01T23:59:35","","Completed","2018-12-24T23:59:35","No","No","No","Internal"]
[null,null,null,4426,null,"24_25/10/2019 9:20:44 AM","2018-12-24T23:59:35","Defect","Ship Staff","Ship Staff Insp.","2S COT PV vlave leaks from pressure side.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.21","High","","","Replaced with overhauled spare.","2019-01-01T23:59:35","","Completed","2018-12-24T23:59:35","No","No","No","Internal"]
[null,null,null,4430,null,"24_25/10/2019 9:35:19 AM","2018-12-24T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Mooring winch No. 1, Aft drum(B), brake cylinder in poor condition.","Deck - Mooring Machinery","Mooring","Equipment Related","9.15","Medium","","","Power tooled and investigate, condition found satisfactory without leaks. Painted and re-fitted.","2019-01-13T23:59:35","","Completed","2018-12-29T23:59:35","No","No","No","Internal"]
[null,null,null,4411,null,"24_25/10/2019 7:55:25 AM","2018-12-25T23:59:35","Defect","Ship Staff","Ship Staff Insp.","PV valve of SLOP P pressure and vacuum side leaks","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.21","High","","","Overhauled and replaced with spare.","2019-01-13T23:59:35","","Completed","2019-01-12T23:59:35","No","No","No","Internal"]
[null,null,null,4412,null,"24_25/10/2019 8:05:54 AM","2018-12-25T23:59:35","Defect","Ship Staff","Ship Staff Insp.","PV valve of 1C COT pressure and vacuum side leaks.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.21","High","","","To replace with overhauled spare.","2019-01-18T23:59:35","","Completed","2019-01-13T23:59:35","No","No","No","Internal"]
[null,null,null,4413,null,"24_25/10/2019 8:08:46 AM","2018-12-25T23:59:35","Defect","Ship Staff","Ship Staff Insp.","PV valve of 2C COT pressure and vacuum side leaks.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.21","High","","","To replace with overhauled spare.","2019-01-13T23:59:35","","Completed","2019-01-17T23:59:35","No","No","No","Internal"]
[null,null,null,4416,null,"24_25/10/2019 7:36:35 AM","2018-12-25T23:59:35","Defect","Ship Staff","Ship Staff Insp.","PV valves slop starboard pressure and vacuum side leaks","Cargo Mach.,Deck - Pipe / Fittings,Inert Gas","Cargo / Ballast Systems","Equipment Related","8.21","High","","","Overhauled and replaced with spare one.","2019-01-13T23:59:35","","Completed","2019-01-05T23:59:35","No","No","No","Internal"]
[null,null,null,4466,null,"24_25/10/2019 11:04:45 AM","2018-12-25T23:59:35","Defect","Ship Staff","Ship Staff Insp.","FGDS pumproom system calibration gas exhausted.","Accommodation","Cargo / Ballast Systems","Human Error","8.46","Very High","","","RO raised and received. Bottle renewed.","2019-05-22T23:59:35","DBAU180221","Completed","2019-04-21T23:59:35","No","No","No","Internal"]
[null,null,null,4471,null,"24_25/10/2019 11:20:23 AM","2018-12-28T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Service air compressor air radiator leaking.","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Received new compressor on 26th Mar 2019 and installed, working satisfactory.","2019-05-11T23:59:35","","Completed","2019-05-12T23:59:35","No","No","No","Internal"]
[null,null,null,4427,null,"24_25/10/2019 9:23:56 AM","2019-01-06T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Port provision crane emergency stop valve frozen.","Deck - Machinery","Structural Condn. / WT integrity ","Equipment Related","11.8","Low","","","Planned to lubricate and free up, if required to be removed and overhauled.","2019-01-13T23:59:35","","Completed","2019-01-08T23:59:35","No","No","No","Internal"]
[null,null,null,4428,null,"24_25/10/2019 9:28:11 AM","2019-01-06T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Stbd Accommodation ladder angle indicator marker missing.","Deck - Machinery","ISM Related","Human Error","5.47","Medium","","","Fabricate and re-fitted in place.","2019-01-13T23:59:35","","Completed","2019-01-13T23:59:35","No","No","No","Internal"]
[null,null,null,4429,null,"24_25/10/2019 9:31:51 AM","2019-01-06T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Stbd Accommodation ladder 1 Nos. step found cracked.","Deck - Machinery","Structural Condn. / WT integrity ","Equipment Related","5.47","Medium","","","Removed, refabricate and fitted back in place.","2019-01-13T23:59:35","","Completed","2019-01-13T23:59:35","No","No","No","Internal"]
[null,null,null,9552,null,"24_07/01/2020 11:02:00 AM","2019-01-10T23:59:35","Non Conformity","Ship Staff","Ship Staff Insp.","Fire line Pressure gauge found defective on port side bridge wing. Gauge was renewed and found in order on 19 Jan 2019.","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.35","Medium","","","Fire line pressure gauge was renewed and verified for operational condition","2019-01-13T23:59:35","","Completed","2019-01-10T23:59:35","No","No","No","Internal"]
[null,null,null,4414,null,"24_25/10/2019 8:10:58 AM","2019-01-26T23:59:35","Defect","Ship Staff","Ship Staff Insp.","PV valve of 3C COT pressure and vacuum side laeks.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.21","High","","","To replace with overhauled spare.","2019-01-31T23:59:35","","Completed","2019-01-29T23:59:35","No","No","No","Internal"]
[null,null,null,4415,null,"24_25/10/2019 8:13:13 AM","2019-01-26T23:59:35","Defect","Ship Staff","Ship Staff Insp.","PV valve of 4C COT pressure and vacuum side leaks.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.21","High","","","To replace with overhauled spare.","2019-01-31T23:59:35","","Completed","2019-01-30T23:59:35","No","No","No","Internal"]
[null,null,null,4417,null,"24_25/10/2019 8:21:35 AM","2019-01-26T23:59:35","Defect","Ship Staff","Ship Staff Insp.","PV valve of 5C pressure and vacuum side leaks.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.21","High","","","To replace with overhauled spare.","2019-02-01T23:59:35","","Completed","2019-01-30T23:59:35","No","No","No","Internal"]
[null,null,null,4470,null,"24_25/10/2019 11:18:19 AM","2019-01-26T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Mooring winch brake cylinder wasted and holed - M5,M6,M7 & M8.","Deck - Mooring Machinery","Mooring","Equipment Related","9.15","Medium","","","Repaired temporarily by welding doubler in E/R workshop. Spares received on 29th Apr 2019 nad replaced defective brake cylinders.","2019-05-11T23:59:35","DBAU190057","Completed","2019-05-12T23:59:35","No","No","No","Internal"]
[null,null,null,4440,null,"24_25/10/2019 10:29:35 AM","2019-02-04T23:59:35","Defect","Ship Staff","Ship Staff Insp.","ME fuel oil supplu pump No.1 mechanical seal leaking.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.2","Low","","","To replace the mechanical seal.","2019-03-01T23:59:35","V-DBAU012685/19","Completed","2019-03-24T23:59:35","No","No","No","Internal"]
[null,null,null,4449,null,"24_25/10/2019 10:52:58 AM","2019-02-04T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Slop port steam return line corroded and holed.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.15","High","","","Repaired with the soft patch temporarily, planned to remove and repair by renewing the pipe in E/R Workshop.","2019-02-17T23:59:35","","Completed","2019-04-20T23:59:35","No","No","No","Internal"]
[null,null,null,4419,null,"24_25/10/2019 8:38:24 AM","2019-02-05T23:59:35","Defect","Ship Staff","Ship Staff Insp.","EGB Manometer missing.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","New manometer fabricated and fitted, Work no. V-DBAU012212/19","2019-03-06T23:59:35","","Completed","2019-02-17T23:59:35","No","No","No","Internal"]
[null,null,null,4420,null,"24_25/10/2019 8:42:04 AM","2019-02-05T23:59:35","Defect","Ship Staff","Ship Staff Insp.","HFO purifier feed pump No.1 mechanical seal leaking.","E/R - Purifier","Eng. / Strg. Comp.","Equipment Related","10.2","Low","","","Overhauled the pump and renewed the mechanical seal.","2019-03-01T23:59:35","JOB NO. DBAU012245/19","Completed","2019-02-11T23:59:35","No","No","No","Internal"]
[null,null,null,4435,null,"24_25/10/2019 10:15:52 AM","2019-02-05T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ME Unit 7 punture valve slightly leaking.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Tightened the punture valve to torque, presently no leaks and under observation.","2019-02-24T23:59:35","","Completed","2019-03-17T23:59:35","No","No","No","Internal"]
[null,null,null,4442,null,"24_25/10/2019 10:35:12 AM","2019-02-05T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Aft winch system hydraulic tank level gauge blanked off with steel pipe.","Miscellaneous","Mooring","Human Error","10.25","Very High","","","Received spares, steel wires renewal in progress. Gauge glass will be renewed after mooring winch works are completed.","2019-03-06T23:59:35","V-DBAU012774/19","Completed","2019-03-27T23:59:35","No","No","No","Internal"]
[null,null,null,4418,null,"24_25/10/2019 8:33:18 AM","2019-02-08T23:59:35","Defect","Ship Staff","Ship Staff Insp.","1S Bunker tank heating coils 3 nos found leaking.","E/R - Pipes/ valves & fittings","Structural Condn. / WT integrity ","Equipment Related","10.32","Very High","","","Added in REFMAN to be done at Dry dock.","2019-12-22T23:59:35","Refman no. BA/SDR/16","Completed","2019-02-14T23:59:35","Yes","No","No","Internal"]
[null,null,null,4421,null,"24_25/10/2019 9:06:06 AM","2019-02-08T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Control air dryer water drain unit leaking.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.19","Very High","","","Overhauled and found working satisfactory.","2019-03-22T23:59:35","JOB NO. DBAU0122452/19","Completed","2019-02-13T23:59:35","No","No","No","Internal"]
[null,null,null,4422,null,"24_25/10/2019 9:08:43 AM","2019-02-08T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Deck valve hydraulic box aft of port manifold found leaking.","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","Equipment Related","8.11","Medium","","","Leakage Rectified.","2019-04-21T23:59:35","JOB NO. DBAU012246/19","Completed","2019-02-20T23:59:35","No","No","No","Internal"]
[null,null,null,4446,null,"24_25/10/2019 10:46:25 AM","2019-02-08T23:59:35","Defect","Ship Staff","Ship Staff Insp.","EGB mild leak observed near water inlet header.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Lagging removed and inspected. Cold work carried out for the corroded section. L-5cm, B-0.5cm.","2019-03-22T23:59:35","","Completed","2019-04-07T23:59:35","No","No","No","Internal"]
[null,null,null,4465,null,"24_25/10/2019 11:01:50 AM","2019-02-08T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Port hose handling crane found to give noise at 45 degrees.","Deck - Machinery","Cargo / Ballast Systems","Equipment Related","8.5","Very High","","","Greasing carried out, found the noise to reduce.","2019-04-21T23:59:35","","Completed","2019-04-21T23:59:35","No","No","No","Internal"]
[null,null,null,9553,null,"24_07/01/2020 11:08:11 AM","2019-02-14T23:59:35","Non Conformity","Ship Staff","Ship Staff Insp.","While topping up SCBA bottles after drill, Found one of SCBA bottle leaking from connector assembly.  After inspection found one of SCBA bottle valve was not holding. When cylinder valve was opened found valve bearing was worn out.","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.43","High","","","Req DBAU190036 was raised for new SCBA bottle valve. Same was received in Singapore on 3rd March. New valve was fitted and leakage was rectified. on 4th Mar 2019.","2019-02-24T23:59:35","","Completed","2019-02-23T23:59:35","No","No","No","Internal"]
[null,null,null,4443,null,"24_25/10/2019 10:37:50 AM","2019-02-14T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Hinges of compactor room door found wasted and broken.","Deck - Pipe / Fittings","General Appearance","Behaviour Based","11.8","Low","","","Door to be dismantled and taken to E/R workshop and repair by welding.","2019-03-21T23:59:35","","Completed","2019-03-31T23:59:35","No","No","No","Internal"]
[null,null,null,4425,null,"24_25/10/2019 9:18:43 AM","2019-02-18T23:59:35","Defect","Ship Staff","Ship Staff Insp.","10-6k steam relief valve found leaking mildly.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Opened the relief valve, lapped and boxed back, found no leaks.","2019-04-06T23:59:35","V-DBAU012091/19","Completed","2019-03-05T23:59:35","No","No","No","Internal"]
[null,null,null,9554,null,"24_07/01/2020 11:10:53 AM","2019-03-01T23:59:35","Non Conformity","Ship Staff","Ship Staff Insp.","During weekly accommodation inspection it was found that the fire door on D-Deck did not close completely after releasing the electro magnetic switch. Door hinges had become loose as a result of which fire door could not be closed completely. ","Accommodation ","Structural Condn. / WT integrity ","Equipment Related","5.35","Medium","","","Door hinges were made tight and fire door can be closed completely. All fire doors were inspected and found in satisfactory condition.","2019-03-04T23:59:35","","Completed","2019-03-02T23:59:35","No","No","No","Internal"]
[null,null,null,4424,null,"24_25/10/2019 9:14:57 AM","2019-03-04T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Hotwell observation tank glass looks dirty.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Opened the tank and cleaning carried out.","2019-05-06T23:59:35","V-DBAU001487/17","Completed","2019-03-05T23:59:35","No","No","No","Internal"]
[null,null,null,4397,null,"24_25/10/2019 10:56:07 AM","2019-03-06T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Lub oil consumption for NO.2 high at 50 L/day.","E/R - Aux. Engine","Eng. / Strg. Comp.","Human Error","10.32","Very High","","","Indicated lub. oil leakage through cyclinder head guides or vents chocked or any external leakage to check and rectify.","2019-03-21T23:59:35","","Completed","2019-04-17T23:59:35","No","No","No","Internal"]
[null,null,null,4423,null,"24_25/10/2019 9:12:24 AM","2019-03-06T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Observed steam continously venting - waste of steam/water.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Cleaned the atmospheric condenser tubes and found the steam venting to reduce.","2019-03-11T23:59:35","V-DBAU000514/17","Completed","2019-03-06T23:59:35","No","No","No","Internal"]
[null,null,null,4431,null,"24_25/10/2019 10:03:17 AM","2019-03-06T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Package galley AC unit in AC compressor room, the suction filter seems chocked.","Miscellaneous","MLC Related","Human Error","11.13","Low","","","Cleaned the suction air filter satisfactorily.","2019-03-21T23:59:35","v-dbau012522/19","Completed","2019-03-09T23:59:35","No","No","No","Internal"]
[null,null,null,4432,null,"24_25/10/2019 10:07:06 AM","2019-03-06T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","AC intake filter fine mesh missing.","Accommodation","MLC Related","Human Error","11.13","Low","","","Fine mesh filter installed.","2019-03-21T23:59:35","V-DBAU012523/19","Completed","2019-03-09T23:59:35","No","No","No","Internal"]
[null,null,null,4433,null,"24_25/10/2019 10:10:40 AM","2019-03-06T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Cable tray anchor bolts painted over.","Deck - Pipe / Fittings","General Appearance","External Factors","11.1","High","","","Anchor bolts should be free and well greased - allowing free movements.","2019-03-16T23:59:35","","Completed","2019-03-15T23:59:35","No","No","No","Internal"]
[null,null,null,4434,null,"24_25/10/2019 10:12:49 AM","2019-03-06T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Fwd liferafts stwing cradles rusted.","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.29","High","","","To de-rust and paint.","2019-03-21T23:59:35","","Completed","2019-03-15T23:59:35","No","No","No","Internal"]
[null,null,null,4436,null,"24_25/10/2019 10:18:44 AM","2019-03-06T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","No. 1 oil max filter found not in use, while engine was running.","E/R - Aux. Engine","Eng. / Strg. Comp.","Human Error","10.32","Very High","","","To ensure the centrifugal filter is always in use while running and while in idle.","2019-03-11T23:59:35","V-DBAU012618/19","Completed","2019-03-20T23:59:35","No","No","No","Internal"]
[null,null,null,4437,null,"24_25/10/2019 10:22:38 AM","2019-03-06T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","No. 1 & 2 lub oil purifier was running, inlet set temperature at 85 deg C, and actual temperature was only 65 deg C.","E/R - Purifier","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Later understood temperature controller not working on auto - neither reported nor in DDRL, to check and revert status.","2019-03-21T23:59:35","V-DBAU012671/19","Completed","2019-03-20T23:59:35","No","No","No","Internal"]
[null,null,null,4438,null,"24_25/10/2019 10:25:03 AM","2019-03-06T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","No.1 & 2 HFO Purifier was running, inlet set temp at 98 deg C and actual temp was only 83 deg C.","E/R - Purifier","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Later understood temp controller was not working on auto - neither reported nor in DDRL, to check and revert status.","2019-03-21T23:59:35","V-DBAU012669/19","Completed","2019-03-20T23:59:35","No","No","No","Internal"]
[null,null,null,4439,null,"24_25/10/2019 10:27:38 AM","2019-03-06T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Few units shall be due for decarb in another 3000 hrs.","E/R - Main Engine","Eng. / Strg. Comp.","Knowledge Based","10.12","Very High","","","To raise RO and maintain sufficient spares for the units falling due +3 sets extra.","2019-04-06T23:59:35","DBAU190098","Completed","2019-03-24T23:59:35","No","No","No","Internal"]
[null,null,null,4441,null,"24_25/10/2019 10:32:00 AM","2019-03-06T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Both boiler gauge glass cocks remote valves not free.","E/R - Boiler","Eng. / Strg. Comp.","Human Error","10.32","Very High","","","Wires greased, leaking packing renewed. Need to ease up the cocks for free movement.","2019-03-21T23:59:35","V-DBAU012767/19, V-DBAU012768/19","Completed","2019-03-25T23:59:35","No","No","No","Internal"]
[null,null,null,4444,null,"24_25/10/2019 10:40:44 AM","2019-03-06T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Fwd light mast stays found fully rusted - devoid of grease.","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","Human Error","11.8","Low","","","To ensure they are well lubricated to avoid strand damages.","2019-03-16T23:59:35","","Completed","2019-03-28T23:59:35","No","No","No","Internal"]
[null,null,null,4445,null,"24_25/10/2019 10:42:45 AM","2019-03-06T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Stern light junction box base plate corroded.","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","External Factors","11.8","Low","","","To renew the base plate.","2019-03-27T23:59:35","","Completed","2019-04-01T23:59:35","No","No","No","Internal"]
[null,null,null,4447,null,"24_25/10/2019 10:48:35 AM","2019-03-06T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Control air compressor external cooling fan kept for radiator.","E/R - Air Comp.","Eng. / Strg. Comp.","Human Error","10.32","Very High","","","Radiator cleaned and external fan removed from place.","2019-03-21T23:59:35","","Completed","2019-03-09T23:59:35","No","No","No","Internal"]
[null,null,null,4448,null,"24_25/10/2019 10:50:29 AM","2019-03-06T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Light glass fully dirty.","Deck - Pipe / Fittings","General Appearance","Human Error","11.9","Low","","","To clean all stern light globes/glasses and fit back.","2019-03-21T23:59:35","V-DBAU012944/19","Completed","2019-04-02T23:59:35","No","No","No","Internal"]
[null,null,null,4464,null,"24_25/10/2019 10:58:05 AM","2019-03-06T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Mooring spring winches brake band stopper bolts clearance found less.","Deck - Machinery","Mooring","External Factors","9.15","Medium","","","To adjust and to maintain around 5mm.","2019-03-16T23:59:35","","Completed","2019-04-21T23:59:35","No","No","No","Internal"]
[null,null,null,4467,null,"24_25/10/2019 11:09:10 AM","2019-03-06T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","IGG operation not checked for long time.","Inert Gas","Cargo / Ballast Systems","Human Error","10.32","Very High","","","PI controller found not working satisfactory, same cheked and found few control air lines leaking, same rectified. ","2019-05-11T23:59:35","V-DBAU013309/19","Completed","2019-05-01T23:59:35","No","No","No","Internal"]
[null,null,null,4469,null,"24_25/10/2019 11:15:18 AM","2019-03-06T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Provision crane - Boom rest pad/platform rusty.","Deck - Machinery","Structural Condn. / WT integrity ","Equipment Related","11.8","Low","","","De-rusted and pinted.","2019-05-11T23:59:35","","Completed","2019-05-12T23:59:35","No","No","No","Internal"]
[null,null,null,4480,null,"24_25/10/2019 12:20:30 PM","2019-03-06T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Incinerator exhaust blower vent controller defective.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Exhaust blower vent controller replaced, tried out. Sludge incineration tried out. Alarms and trips tested, working satisfactory.","2019-05-25T23:59:35","","Completed","2019-05-23T23:59:35","No","No","No","Internal"]
[null,null,null,4487,null,"24_25/10/2019 12:26:21 PM","2019-03-06T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","U-Clamps on the IG line  - at china passage rusted and wasted.","Deck - Pipe / Fittings","General Appearance","External Factors","11.4","Very High","","","U-Clamps replaced. De-rusting and painting of support angle bars carried out.","2019-06-06T23:59:35","","Completed","2019-05-28T23:59:35","No","No","No","Internal"]
[null,null,null,4488,null,"24_25/10/2019 1:06:39 PM","2019-03-06T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","All hydraulic valve boxes hinges packing channels rusty.","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","Equipment Related","11.3","Medium","","","Channels de-rusted and painted.","2019-06-06T23:59:35","","Completed","2019-06-05T23:59:35","No","No","No","Internal"]
[null,null,null,9555,null,"24_07/01/2020 11:20:08 AM","2019-03-31T23:59:35","Non Conformity","Ship Staff","Ship Staff Insp.","Anemometer on bridge / repeater in CCR not fitted with alarm limits  functions. No recorder / printer provided in CCR.","Navigation - Others","Navigation","Equipment Related","4.7","High","","","Wind speed and direction to be continuously monitored in port and logged down hourly by duty officers.","2019-04-09T23:59:35","","Completed","2019-04-17T23:59:35","No","No","No","Internal"]
[null,null,null,9556,null,"24_07/01/2020 11:25:33 AM","2019-03-31T23:59:35","Observation","Ship Staff","Ship Staff Insp.","As required by company policy, following entries not made in Bridge Note book-\n\n1) Berth to berth passage plan is available\n\n2) UKC calculations completed\n\n3) Charts for voyage available, corrected and route plotted\n\n4) Crew notified about time of departur","Documentation","Cert. & Docu.","Human Error","4.1","High","","","All OOW educated regarding minimum entries to be made i bridge note book.","2019-04-09T23:59:35","","Completed","2019-04-08T23:59:35","No","No","No","Internal"]
[null,null,null,9557,null,"24_07/01/2020 11:30:07 AM","2019-03-31T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Gyro error not being checked / recorded prior departure from port","Navigation - Others","Navigation","Human Error","4.9","Medium","","","All OOW instructed to verify gyro error prior departure from port (along with per-departure checks)","2019-04-09T23:59:35","","Completed","2019-04-08T23:59:35","No","No","No","Internal"]
[null,null,null,9558,null,"24_07/01/2020 11:44:51 AM","2019-04-11T23:59:35","Non Conformity","Ship Staff","Ship Staff Insp.","During weekly accommodation rounds it was observed that dangerous sector for the fire doors inside accommodation was not marked. ","Accommodation ","Safety / LSA / FFA","Human Error","5.35","Medium","","","This was brought to the notice of officer in charge and dangerous sector for all the fire doors were marked.","2019-04-21T23:59:35","","Completed","2019-04-20T23:59:35","No","No","No","Internal"]
[null,null,null,4505,null,"24_25/10/2019 2:03:16 PM","2019-04-21T23:59:35","Defect","Ship Staff","Ship Staff Insp.","atmospheric condenser tubes chocked by 47%needs renewal.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","new atmospheric condenser installed in place and put in use.","2019-07-22T23:59:35","DBAU195066","Completed","2019-08-27T23:59:35","No","No","No","Internal"]
[null,null,null,9559,null,"24_07/01/2020 11:51:52 AM","2019-04-29T23:59:35","Non Conformity","Ship Staff","Ship Staff Insp.","Fixed communication system to provide links between the pump room and navigational bridge is not available onboard.","Miscellaneous","Communication","Industry Issue","5.17","Very High","","","1. A risk assessment for Pump room man entry is in place.\n\n2. A reporting interval of 10 minutes is agreed to for persons entering the pump room and same is recorded in the pump room entry permit.\n\n3. The UHF communication between the bridge and pump room has been tested and found to be in order and confirmed to have reliable reception at the bridge.","2019-05-22T23:59:35","","Completed","2019-05-18T23:59:35","No","No","No","Internal"]
[null,null,null,9560,null,"24_07/01/2020 12:44:26 PM","2019-04-29T23:59:35","Non Conformity","Ship Staff","Ship Staff Insp.","Vapor was being hissing out from the pressure side of the high velocity valve of slop tank starboard during discharging at Kiire.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Human Error","8.21","High","","","After departure from discharge port, the PV valve for Slop Stbd was replaced\n\nwith a spare PV valve which had been tested and kept as standby.\n\nThe Slop Stbd PV Valve which was removed from location, was inspected and pressure side seat\n\nwas cleaned. The PV valve was thereafter tested using the PV Valve test kit and confirmed to be\n\nholding to the designed pressure.","2019-05-02T23:59:35","","Completed","2019-05-01T23:59:35","No","No","No","Internal"]
[null,null,null,9561,null,"24_07/01/2020 12:48:58 PM","2019-04-29T23:59:35","Non Conformity","Ship Staff","Ship Staff Insp.","When testing the steering gear in the emergency mode (#1 steer\n\ngear), it was observed rudder could not stand at certain position and continuously tend to\n\nmove to starboard side.","Elect. Mach. & Equip.","Emgcy. Systems","Equipment Related","10.39","High","","","The root cause was immediately identified and the position of the adjusting pin was corrected\n\nto the neutral set point. The steering gear system was tried out in emergency mode as well as\n\nin normal mode and found to be operating satisfactory, with the rudder angle remaining\n\nstationary as per the desired position.","2019-05-22T23:59:35","","Completed","2019-04-30T23:59:35","No","No","No","Internal"]
[null,null,null,9571,null,"24_07/01/2020 12:56:27 PM","2019-04-29T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Mooring system management plan indicated that the vessels Ship\n\nDesign MBL was 115 tons. However, SWL of mooring bitts on forecastle (2 sets) and on poop\n\ndeck (4 sets) were marked as 74 tons (less than the Ship Design MBL).","Deck - Mooring Machinery","Structural Condn. / WT integrity ","Industry Issue","9.19","Low","","","Vessel confirm that the ship’s winch mounted lines and associated closed chocks are\n\nprovided basis the ship design MBL of 115 Ton.","2019-05-22T23:59:35","","Completed","2019-05-17T23:59:35","No","No","No","Internal"]
[null,null,null,4479,null,"24_25/10/2019 12:17:45 PM","2019-04-29T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Local fire fighting alarn control panel : push button defective","Critical Equip.","ISM Related","Equipment Related","5.39","Very High","","","RO received ON 25 MAY 2019. Office concurrence taken and push button replaced. Test carried out in Incinerator area. Working satisfactory. Hypermist system put back in auto mode.","2019-05-22T23:59:35","DBAU190080, V-DBAU013666/19","Completed","2019-05-21T23:59:35","No","No","No","Internal"]
[null,null,null,8064,null,"24_Wed Jun 12 2019 00:36:28 GMT+0000 (Coordinated Universal Time)","2019-04-29T23:59:35","Defect","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","It was observed that a communication system to provide links between the pump room and navigation bridge was not available at the time of inspection.","Navigation - GMDSS & Communication","Communication","Inappropriate Procedure","5.17","Very High","","","1. A risk assessment for Pump room man entry is in place.\n\n2. A reporting interval of 10 minutes is agreed to for persons entering the pump room and same is recorded in the pump room entry permit.\n\n3. The UHF communication between the bridge and pump room has been tested and found to be in order and confirmed to have reliable reception at the bridge.\n\nOffice has planned to install passive antennas on board to enhance the UHF communication system between the pump room and navigational bridge and to make it more reliable. Included in DD specs - REFMAN.","2019-05-25T23:59:35","","Completed","2019-05-18T23:59:35","No","No","No","External"]
[null,null,null,8065,null,"24_Wed Jun 12 2019 00:39:52 GMT+0000 (Coordinated Universal Time)","2019-04-29T23:59:35","Defect","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","Vapour was being hissing out from the pressure side of the high velocity valve of slop tank starboard at the time of the inspection.","Cargo Mach.,Deck - Machinery","Cargo / Ballast Systems","Equipment Related","8.21","High","","","After departure from discharge port, the PV valve for Slop Stbd was replaced\n\nwith a spare PV valve which had been tested and kept as standby.\n\nThe Slop Stbd PV Valve which was removed from location, was inspected and pressure side seat\n\nwas cleaned. The PV valve was thereafter tested using the PV Valve test kit and confirmed to be\n\nholding to the designed pressure.\n\nAfter carrying out the function test of PV vavle crew members must ensure that the seat of high velocity vent valve is clean and clear of any debris. After the function test is over crew member should check if the PV valve has reset correctly and no leaks are observed.\n\n","2019-05-25T23:59:35","","Completed","2019-05-01T23:59:35","No","No","No","External"]
[null,null,null,8066,null,"24_Wed Jun 12 2019 00:43:26 GMT+0000 (Coordinated Universal Time)","2019-04-29T23:59:35","Defect","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","Mooring system management plan indicated that the ships design MBL was 115 T, however the SWL of mooring bit on forecastle (2 set) and on poop deck (4 set) were marked as 74 T (Less than ships design MBL)","Deck - Machinery","Mooring","Industry Issue","9.19","Low","","","Vessel confirm that the ship’s winch mounted lines and associated closed chocks are\n\nprovided basis the ship design MBL of 115 Ton.\n\nThe ship staff made aware that the mooring bitts as indicated in the observation are of 74 Ton SWL\n\nand this is addressed in the vessel specific “Mooring System Management Plan and Line\n\nManagement Plan”.\n\n","2019-05-25T23:59:35","","Completed","2019-05-17T23:59:35","No","No","No","External"]
[null,null,null,8067,null,"24_Wed Jun 12 2019 00:47:31 GMT+0000 (Coordinated Universal Time)","2019-04-29T23:59:35","Defect","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","When testing the steering gear in emergency mode, (No. 1 steering gear ), it was observed the rudder could not stand at certain position and continuously tend to move to starboard side.","Navigation - Others","Eng. / Strg. Comp.","Equipment Related","10.39","High","","","The root cause was immediately identified and the position of the adjusting pin was corrected\n\nto the neutral set point. The steering gear system was tried out in emergency mode as well as\n\nin normal mode and found to be operating satisfactory, with the rudder angle remaining\n\nstationary as per the desired position.\n\nThe ship staff have been advised that during emergency steering drills, it should be confirmed\n\nthat the rudder is holding position. This check has been included in the Job description for the 3\n\nmonthly Emergency Steering Gear Test.","2019-05-25T23:59:35","","Completed","2019-04-30T23:59:35","No","No","No","External"]
[null,null,null,4477,null,"24_25/10/2019 11:35:17 AM","2019-05-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","No.2 COPT speed control governer switch in CCR to replace as defective.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","10.32","Very High","","","Replaced and tested.","2019-05-22T23:59:35","V-DBAU013589/19","Completed","2019-05-19T23:59:35","No","No","No","Internal"]
[null,null,null,4484,null,"24_25/10/2019 12:55:26 PM","2019-05-01T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Grey water line modification.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","External Factors","10.32","Very High","","","Consumable recived 25 MAY 2019, job completed, drawings, photos and permits added in PAL.","2019-06-06T23:59:35","V-DBAU013871/19","Completed","2019-06-01T23:59:35","No","No","No","Internal"]
[null,null,null,4485,null,"24_25/10/2019 12:58:04 PM","2019-05-02T23:59:35","Defect","Ship Staff","Suptd. Insp.","ME OMD : to replace PCB due to message in screen\"Replace EEPROM\"","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.21","Medium","","","PCB replaced and tested, working satisfactory.","2019-06-06T23:59:35","V-DBAU013903/19","Completed","2019-06-04T23:59:35","No","No","No","Internal"]
[null,null,null,4468,null,"24_25/10/2019 11:13:18 AM","2019-05-03T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Stern tube Lub. oil flow meter defective.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","RO raised and recived, same fitted.","2019-05-03T23:59:35","V-DBAU013360/19","Completed","2019-05-03T23:59:35","No","No","No","Internal"]
[null,null,null,4400,null,"24_25/10/2019 3:11:11 PM","2019-05-06T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Galley exhaust fan breaker-reset button defective.","Elect. Mach. & Equip.","General Appearance","Equipment Related","10.37","Medium","","","No action required. As per design, reset button is inside the panel ( not outside). Ther is no mechanism connected inside switch to outside knob. Any reset required os to be done from inside by design.","2020-01-23T23:59:35","DNAU190131","Completed","2020-03-01T23:59:35","No","No","No","Internal"]
[null,null,null,4500,null,"24_25/10/2019 1:45:57 PM","2019-05-06T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Hooter for E/R bottom platform not working.","Miscellaneous","Eng. / Strg. Comp.","External Factors","10.37","Medium","","","Hooter renewed with the spare.","2019-08-23T23:59:35","V-DBAU014924/19, DBAU190133","Completed","2019-07-27T23:59:35","No","No","No","Internal"]
[null,null,null,4478,null,"24_25/10/2019 11:37:13 AM","2019-05-08T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Fresh water generator ejector pump discharge valve to replcae as corroded.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.31","Very High","","","Spares recived on 25th May 2019. Valve replaced and put in service.","2019-05-21T23:59:35","V-DBAU13626/19","Completed","2019-05-21T23:59:35","No","No","No","Internal"]
[null,null,null,9562,null,"24_07/01/2020 1:02:18 PM","2019-05-10T23:59:35","Non Conformity","Ship Staff","Ship Staff Insp.","During the weekly accommodation inspection oil soaked and dirty boiler suit was found in one of the crew cabin","Accommodation ","General Appearance","Human Error","11.13","Low","","","Crew member was informed and dirty boiler suit was removed from his cabin. The incident was discussed among all crew members and maintaining personnel and ship's hygiene was emphasized on.","2019-05-10T23:59:35","","Completed","2019-05-10T23:59:35","No","No","No","Internal"]
[null,null,null,4472,null,"24_25/10/2019 11:24:05 AM","2019-05-12T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","No. 2 AC Compressor cyclinder head and pistons to inspect due to abnormal noise.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Play in port bank fwd piston gudgeon pin bush. All pistons, cylinder heads checked and spares replaced. Sump oil renewed, working satisfactory.","2019-05-12T23:59:35","V-DBAU013548/19","Completed","2019-05-12T23:59:35","No","No","No","Internal"]
[null,null,null,4475,null,"24_25/10/2019 11:31:07 AM","2019-05-13T23:59:35","Defect","Ship Staff","Ship Staff Insp.","No.1 Aux Boiler FD fan air intake trunking crack to weld.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Cracked area gouged and welded. Boiler tried out and no leaks noted.","2019-05-15T23:59:35","","Completed","2019-05-15T23:59:35","No","No","No","Internal"]
[null,null,null,4493,null,"24_25/10/2019 1:23:20 PM","2019-05-13T23:59:35","Defect","Ship Staff","Ship Staff Insp.","BHC indication plate of varios mooring winches heavily corroded.","Deck - Mooring Machinery","Mooring","Equipment Related","9.7","Medium","","","New plates for BHC fabricated and fixed back.","2019-07-06T23:59:35","","Completed","2019-06-10T23:59:35","No","No","No","Internal"]
[null,null,null,4473,null,"24_25/10/2019 11:26:33 AM","2019-05-15T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Port provision crane found to make noise during luffing operation due to worn out flange bearing.","Deck - Machinery","Structural Condn. / WT integrity ","Equipment Related","11.8","Low","","","Added in REFMAN.","2019-11-21T23:59:35","","Completed","2019-05-15T23:59:35","Yes","No","No","Internal"]
[null,null,null,4474,null,"24_25/10/2019 11:28:49 AM","2019-05-15T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Atmospheric condenser sea water outlet line after the valve needs to be renewed with rubber coating.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Added in REFMAN.","2019-11-21T23:59:35","","Completed","2019-05-15T23:59:35","Yes","No","No","Internal"]
[null,null,null,4476,null,"24_25/10/2019 11:33:20 AM","2019-05-17T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Hose handling crane (port) : replace valve block No.104","Deck - Machinery","Structural Condn. / WT integrity ","Equipment Related","8.5","Very High","","","Replaced valve block.","2019-05-21T23:59:35","DBAU195047","Completed","2019-05-19T23:59:35","No","No","No","Internal"]
[null,null,null,4401,null,"24_25/10/2019 3:13:47 PM","2019-05-18T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Ballast pump #2 : Auto grease cup to replace.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","SPARE RECEIVED IN SINGAPORE, USED TO REPLACE THE DEFECTIVE GREASE CUP","2019-10-23T23:59:35","DBAU190138","Completed","2019-11-16T23:59:35","No","No","No","Internal"]
[null,null,null,4497,null,"24_25/10/2019 1:32:56 PM","2019-05-18T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","Control Air compresser : pin hole in the air cooler.","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Leak identified and arrested.","2019-07-06T23:59:35","V-DBAU013128/19","Completed","2019-06-23T23:59:35","No","No","No","Internal"]
[null,null,null,4481,null,"24_25/10/2019 12:23:36 PM","2019-05-24T23:59:35","Defect","Ship Staff","Ship Staff Insp.","AE#3 : Air cooler to pressure test FW side as leaking","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Air cooler removed, chemically cleaned, pressure tested, tube plugged, boxed back and put in service. No leaks in system.","2019-06-01T23:59:35","","Completed","2019-05-26T23:59:35","No","No","No","Internal"]
[null,null,null,4482,null,"24_25/10/2019 12:50:26 PM","2019-05-29T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","AE#1,2,3 : Alternator side to clean with air and chemical.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Added to REFMAN.","2019-11-21T23:59:35","","Completed","2019-05-29T23:59:35","Yes","No","No","Internal"]
[null,null,null,4483,null,"24_25/10/2019 12:52:58 PM","2019-05-29T23:59:35","Defect","Ship Staff","Ship Staff Insp.","AE#1 : Mechanical overspeed mechnism to replace, dur to not operational while testing of alarms and trips(routine).","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Replaced with spare overspeed mechnism, tried out, working satisfactory.","2019-05-29T23:59:35","V-DBAU013804/19","Completed","2019-05-29T23:59:35","No","No","No","Internal"]
[null,null,null,4486,null,"24_25/10/2019 1:02:15 PM","2019-06-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","FW Generator : Evaporator bottom cover to remove as corroded in a section area, due to sea water seepage.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.31","Very High","","","Bottom and cover removed, found section area corroded (about 40 mm hole). Ingress of seawater dur to damage of rubber coating section area inserted, welded and fitted back. ","2019-06-06T23:59:35","V-DBAU013930/19","Completed","2019-06-05T23:59:35","No","No","No","Internal"]
[null,null,null,4489,null,"24_25/10/2019 1:10:43 PM","2019-06-07T23:59:35","Defect","Ship Staff","Ship Staff Insp.","E/R Ventilation dampers actuators to replace as air sealing bushers/o-rings leaking. ","LSA / FFA","Safety / LSA / FFA","Equipment Related","10.32","Very High","","","Acutators received, same replaced and tested, working satisfactory.","2019-06-21T23:59:35","V-DBAU014044/19","Completed","2019-06-11T23:59:35","No","No","No","Internal"]
[null,null,null,4501,null,"24_25/10/2019 1:48:11 PM","2019-06-10T23:59:35","Defect","Ship Staff","Ship Staff Insp.","E/R Workshop AC : Efficiency low due to under rated evaporator coil.","E/R - Aux. Mach.","MLC Related","Equipment Related","10.32","Very High","","","Workshop AC Evaporator renewed with new one.","2019-07-22T23:59:35","V-DBAU014988/19, DBAU190141","Completed","2019-07-30T23:59:35","No","No","No","Internal"]
[null,null,null,4490,null,"24_25/10/2019 1:13:37 PM","2019-06-12T23:59:35","Defect","Ship Staff","Ship Staff Insp.","ME Fuel oil circulating pump No.1 to overhaul. Found spider coupling damaged and hard to turn during inspection.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Pump overhauled, spider coupling and pump bearing replaced. Mechanical seal in good condition, tried out and working satisfactory.","2019-06-12T23:59:35","V-DBAU014042/19","Completed","2019-06-12T23:59:35","No","No","No","Internal"]
[null,null,null,4491,null,"24_25/10/2019 1:16:41 PM","2019-06-12T23:59:35","Defect","Ship Staff","Ship Staff Insp.","HFO auto backwash filter top cover : renew O-rings and seal as leaking.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Top cover overhauled and replaced O rings and seals. Put back in service.","2019-06-12T23:59:35","V-DBAU014043/19","Completed","2019-06-12T23:59:35","No","No","No","Internal"]
[null,null,null,4494,null,"24_25/10/2019 1:25:53 PM","2019-06-13T23:59:35","Defect","Ship Staff","Ship Staff Insp.","E/R Sunken deck whether tight entrance door(port) hinge pin broken, same to be removed adn fabricated.","Miscellaneous","Eng. / Strg. Comp.","External Factors","11.6","Medium","","","Pin fabricated and fixed back.","2019-06-21T23:59:35","","Completed","2019-06-21T23:59:35","No","No","No","Internal"]
[null,null,null,4502,null,"24_25/10/2019 1:52:14 PM","2019-06-14T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Control air dryer : Control air low pressure. Problem traced to decsiccant, which need to replace every 2 years.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Decsiccant renewed with spare, control air dryer shuttle valve renewed.","2019-07-22T23:59:35","V-DBAU004454/17, DBAU190142","Completed","2019-07-25T23:59:35","No","No","No","Internal"]
[null,null,null,4496,null,"24_25/10/2019 1:30:00 PM","2019-06-18T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Brake cylinder of mooring winch W1A corroded, wasted and holed.","Deck - Mooring Machinery","Mooring","Equipment Related","9.15","Medium","","","Brake cylinder renewed and BHC tested, found satisfactory.","2019-07-03T23:59:35","","Completed","2019-07-01T23:59:35","No","No","No","Internal"]
[null,null,null,9563,null,"24_07/01/2020 1:06:58 PM","2019-06-19T23:59:35","Non Conformity","Ship Staff","Ship Staff Insp.","During abandon ship drill it was observed that   no poster or instruction posted for lifeboat recovery procedure on the upper deck muster stations.","LSA / FFA","Safety / LSA / FFA","Human Error","5.14","Very High","","","Ship specific lifeboat recovery procedures prepared and posted at muster stations on upper deck.","2019-10-21T23:59:35","","Completed","2019-08-10T23:59:35","No","No","No","Internal"]
[null,null,null,4492,null,"24_25/10/2019 1:20:29 PM","2019-06-19T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Incinerator : Combustion chamber thermocouple to replace as defective.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Same replaced, tried out. Found working satisfactory.","2019-06-19T23:59:35","V-DBAU014069/19, DBAU190150","Completed","2019-06-19T23:59:35","No","No","No","Internal"]
[null,null,null,4506,null,"24_25/10/2019 2:07:58 PM","2019-06-19T23:59:35","Defect","Ship Staff","Ship Staff Insp.","various ligthing diffusers needs to be replaceddeffective, wear and tear)","Elect. Mach. & Equip.","Eng. / Strg. Comp.","External Factors","10.15","Low","","","diffusers replaced with spare one.","2019-07-22T23:59:35","DBAU190149","Completed","2019-08-17T23:59:35","No","No","No","Internal"]
[null,null,null,9564,null,"24_07/01/2020 1:12:23 PM","2019-06-20T23:59:35","Non Conformity","Ship Staff","Ship Staff Insp.","After departure load port gangway log book and visitor cards were checked. Upon checking it was found that 5 visitor cards were missing. Same was reported to the master and search for stowaways carried out. Upon completion of search it was concluded that visitors must have taken the visitor cards along with them while disembarking the vessel. Missing visitor card numbers were noted and reported to the office. ","Miscellaneous","ISPS Related","Human Error","7.3","Low","","","Stowaway search was carried out immediately. Upon completion of search it was concluded that visitors must have taken the visitor card with themselves. Office was notified by master immediately. Missing visitor card numbers were noted down and all crew members briefed about the incident and breach of ship' s security.","2019-06-21T23:59:35","","Completed","2019-06-20T23:59:35","No","No","No","Internal"]
[null,null,null,4495,null,"24_25/10/2019 1:28:03 PM","2019-06-22T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Bilge well Stbd : new gratings to fabicate as corroded.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","External Factors","10.29","Medium","","","Gratings fabricated and fixed back.","2019-07-06T23:59:35","V-DBAU002306/17","Completed","2019-07-01T23:59:35","No","No","No","Internal"]
[null,null,null,4399,null,"24_25/10/2019 2:55:41 PM","2019-06-26T23:59:35","Non Conformity","Owner / Marine / Tech. Suptd.","OM Insp. (Eg. SIRE / CDI etc.)","IS telephone system in pump room, donot have a direct connection to Nav Bridge","LSA / FFA","Communication","Industry Issue","5.17","Very High","","","It was clrified that Walkie Talkie as accepted means of communication","2019-12-24T23:59:35","DBAU195057","Completed","2019-12-16T23:59:35","No","No","No","Internal"]
[null,null,null,4498,null,"24_25/10/2019 1:35:24 PM","2019-07-06T23:59:35","Defect","Ship Staff","Ship Staff Insp.","HFO auto backwash filter : leak due to wear down of motor shaft support.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Motor support replaced found no leaks, working satisfactry.","2019-07-06T23:59:35","V-DBAU014592/19","Completed","2019-07-06T23:59:35","No","No","No","Internal"]
[null,null,null,4507,null,"24_25/10/2019 2:11:46 PM","2019-07-11T23:59:35","Defect","Ship Staff","Ship Staff Insp.","LT cooler #2(aft):SW valves not holding, planned to dismantle and clean the plates.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Renewed the valve not holding up.","2019-08-06T23:59:35","DBAU190160","Completed","2019-08-26T23:59:35","No","No","No","Internal"]
[null,null,null,4456,null,"24_25/10/2019 9:21:23 PM","2019-07-12T23:59:35","Defect","Ship Staff","Ship Staff Insp.","AC Compressor No. 2 condenser dryer cartridge was planned for replacement, but the valves are not holding.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Added to refman to be done in DD.","2019-10-11T23:59:35","","Completed","2019-11-08T23:59:35","Yes","No","No","Internal"]
[null,null,null,4450,null,"24_25/10/2019 2:24:19 PM","2019-07-14T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Wheel house telegraph printer-auto roll device defective.","Navigation - Others","Navigation","Equipment Related","4.2","Medium","","","Deffective auto roll device changed.","2019-10-12T23:59:35","DBAU190169","Completed","2019-10-01T23:59:35","No","No","No","Internal"]
[null,null,null,4499,null,"24_25/10/2019 1:43:28 PM","2019-07-14T23:59:35","Defect","Ship Staff","Ship Staff Insp.","No.1 & No.2 bilge fire and GS Pump priming pump engaging cycliner not functioning properly.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","5.38","High","","","Priming unit engaging cylinder removed from place and overhauled.","2019-07-17T23:59:35","","Completed","2019-07-16T23:59:35","No","No","No","Internal"]
[null,null,null,9565,null,"24_07/01/2020 1:17:43 PM","2019-07-18T23:59:35","Non Conformity","Ship Staff","Ship Staff Insp.","During navigation audit on bridge , it was noticed that muster list posted on bridge is different format form the one required by management .  ","Documentation","ISM Related","Human Error","5.13","High","","","Muster list was changed at all the locations with new muster list company specific format.","2019-09-18T23:59:35","","Completed","2019-07-18T23:59:35","No","No","No","Internal"]
[null,null,null,4398,null,"24_25/10/2019 2:43:29 PM","2019-07-20T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Midship darft gauge port side shwoing incorrect reading.","E/R - Aux. Mach.","Structural Condn. / WT integrity ","Equipment Related","11.1","High","","","Span and zero adjustemnt carried out. SAAB and indicator both are showing correct / APPROX. same reading. ","2019-10-22T23:59:35","","Completed","2019-10-19T23:59:35","No","No","No","Internal"]
[null,null,null,4402,null,"24_25/10/2019 3:17:55 PM","2019-07-20T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Midship draft gauge stbd side showing incorrect reading.","Miscellaneous","Cargo / Ballast Systems","Equipment Related","11.1","High","","","Span and zero adjustment carried out. SAAB and indicator both are showing correct / APPROX. same reading.","2019-10-22T23:59:35","","Completed","2019-10-19T23:59:35","No","No","No","Internal"]
[null,null,null,4403,null,"24_25/10/2019 3:21:06 PM","2019-07-20T23:59:35","Defect","Ship Staff","Ship Staff Insp.","2 STBD WBT level not displayed.","Miscellaneous","Cargo / Ballast Systems","Equipment Related","8.12","Medium","","","Troubleshooting carried out, zero calibration done, purging air adjusted.","2019-10-22T23:59:35","","Completed","2019-11-08T23:59:35","No","No","No","Internal"]
[null,null,null,4404,null,"24_25/10/2019 3:23:26 PM","2019-07-20T23:59:35","Defect","Ship Staff","Ship Staff Insp.","3STBD WBT level not displayed.","Miscellaneous","Cargo / Ballast Systems","Equipment Related","8.12","Medium","","","troubleshooting carried out, zero calibration done, and purging air adjusted.","2019-10-22T23:59:35","","Completed","2019-11-08T23:59:35","No","No","No","Internal"]
[null,null,null,4504,null,"24_25/10/2019 1:55:07 PM","2019-07-20T23:59:35","Defect","Ship Staff","Ship Staff Insp.","SAT-C Antenna on aft mast parted from base.","Navigation - GMDSS & Communication","Navigation","Equipment Related","11.8","Low","","","Permanent repair carried out.","2019-08-20T23:59:35","","Completed","2019-08-02T23:59:35","No","No","No","Internal"]
[null,null,null,4508,null,"24_25/10/2019 2:15:11 PM","2019-07-21T23:59:35","Defect","Ship Staff","Ship Staff Insp.","#2 LO purifier :auto operation function not working.","E/R - Purifier","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Heater used from no.1 system, the purifier working satisfactory.","2019-08-21T23:59:35","","Completed","2019-08-07T23:59:35","No","No","No","Internal"]
[null,null,null,4503,null,"24_25/10/2019 1:59:21 PM","2019-07-25T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","air trunking fwd of IGG holed.","Miscellaneous","Eng. / Strg. Comp.","External Factors","10.32","Very High","","","trunking repaired by welding and insert.","2019-08-22T23:59:35","","Completed","2019-07-31T23:59:35","No","No","No","Internal"]
[null,null,null,4405,null,"24_25/10/2019 3:30:44 PM","2019-07-27T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Galley fridge cooling insufficient","Miscellaneous","MLC Related","Equipment Related","11.13","Low","","","Item cancelled as it is found repeted as ( Galley fridge not working) on another defect","2020-01-23T23:59:35","","Completed","2020-04-02T23:59:35","No","No","No","Internal"]
[null,null,null,4460,null,"24_25/10/2019 3:33:17 PM","2019-07-27T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Main engine No.7 unit lubricator leaking","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Lubricator top cover securing bolts tightened.","2019-10-22T23:59:35","","Completed","2019-10-15T23:59:35","No","No","No","Internal"]
[null,null,null,4509,null,"24_25/10/2019 2:18:26 PM","2019-07-27T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Minor leakage from ME unit #7 Exhaust valve jacket water outlet pipe flange","E/R - Main Engine","Eng. / Strg. Comp.","Behaviour Based,Equipment Related","10.29","Medium","","","Gasket renewed, leakage rectified.","2019-09-21T23:59:35","","Completed","2019-08-28T23:59:35","No","No","No","Internal"]
[null,null,null,4406,null,"24_25/10/2019 3:37:10 PM","2019-07-31T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Emergency generator room supply fan indication is not working.","Miscellaneous","Emgcy. Systems","Equipment Related","10.32","Very High","","","Repaires carried out. renwed bulb. working fine now.","2020-01-23T23:59:35","DBAU190177","Completed","2020-02-25T23:59:35","No","No","No","Internal"]
[null,null,null,4451,null,"24_25/10/2019 2:27:33 PM","2019-08-08T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Emergency generator battery is malfunctioning.","LSA / FFA","Emgcy. Systems","Equipment Related","10.34","High","","","Batteries received and installed in place . Engine tried out, starting satisfactory.","2019-11-21T23:59:35","DBAU190174","Completed","2019-10-01T23:59:35","No","No","No","Internal"]
[null,null,null,4452,null,"24_25/10/2019 2:31:09 PM","2019-08-19T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Ligthing diffusers defective in engine room","Elect. Mach. & Equip.","Eng. / Strg. Comp.","External Factors","10.15","Low","","","Engine room ligthing diffusers received on 10th oct.Deffective cracked diffuser in engine room changed with new spare.","2019-12-21T23:59:35","DBAU190190","Completed","2019-10-03T23:59:35","No","No","No","Internal"]
[null,null,null,4457,null,"24_25/10/2019 9:24:10 PM","2019-08-19T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Few of the ballast pumps local pressure gauges in pump room defective","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.8","Medium","","","Added in refman to be done at DD. Gauges ordered.","2019-12-21T23:59:35","DBAU190197","Completed","2019-11-08T23:59:35","Yes","No","No","Internal"]
[null,null,null,4463,null,"24_25/10/2019 2:48:03 PM","2019-08-19T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Few of the ballast pump local pressure gauges defective.","E/R - Aux. Mach.","Structural Condn. / WT integrity ","Behaviour Based","8.5","Very High","","","Added to REFMAN to be done at drydock. ","2019-12-21T23:59:35","DBAU190197","Completed","2019-09-29T23:59:35","Yes","No","No","Internal"]
[null,null,null,4461,null,"24_25/10/2019 3:44:24 PM","2019-08-26T23:59:35","Defect","Ship Staff","Ship Staff Insp.","NO 3 foam monitor leaking , valve not holding.","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.38","High","","","Valve repaired and leakage rectified. Req. cancelled.","2019-10-06T23:59:35","DBAU190188","Completed","2019-10-08T23:59:35","No","No","No","Internal"]
[null,null,null,4462,null,"24_25/10/2019 3:47:20 PM","2019-08-30T23:59:35","Defect","Ship Staff","Ship Staff Insp.","After loading observed PV valve of SLOP S COT leaking from vaccum side.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.21","High","","","replaced by spare overhauled PV valve.","2019-09-21T23:59:35","","Completed","2019-10-07T23:59:35","No","No","No","Internal"]
[null,null,null,4409,null,"24_25/10/2019 3:51:13 PM","2019-09-02T23:59:35","Defect","Ship Staff","Ship Staff Insp.","M3 & M4 mooring winch operating lever valve leaking , brake cylinder valve block leaking.","Deck - Mooring Machinery","Mooring","Equipment Related","9.14","Medium","","","M3, M4,& M5 winchs operating lever blocks overhauled, spare seals and O'rings renewed. Test run carried out. No leaks present now.","2020-01-23T23:59:35","DBAU190205","Completed","2020-03-10T23:59:35","No","No","No","Internal"]
[null,null,null,4453,null,"24_25/10/2019 2:34:40 PM","2019-09-03T23:59:35","Defect","Ship Staff","Ship Staff Insp.","No.2 main fuel oil supply pump has slight leak from seal area .","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","pump overhauled with new seal.","2019-09-21T23:59:35","","Completed","2019-09-10T23:59:35","No","No","No","Internal"]
[null,null,null,4458,null,"24_25/10/2019 3:53:54 PM","2019-09-03T23:59:35","Defect","Ship Staff","Ship Staff Insp.","25kg DCP portable extinguisher (helicopter)","LSA / FFA","Safety / LSA / FFA","Industry Issue","5.42","Medium","","","Repaired and painted. Requisition cancelled.","2019-10-06T23:59:35","DBAU190188","Completed","2019-10-09T23:59:35","No","No","No","Internal"]
[null,null,null,4510,null,"24_25/10/2019 2:21:08 PM","2019-09-03T23:59:35","Defect","Ship Staff","Ship Staff Insp.","No.1 HFO purifier upper hood leaking same need to be replaced.","E/R - Purifier","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Upper hood replaced with new one, tried out found no leak.","2019-09-06T23:59:35","","Completed","2019-09-05T23:59:35","No","No","No","Internal"]
[null,null,null,9566,null,"24_07/01/2020 1:25:34 PM","2019-09-14T23:59:35","Non Conformity","Ship Staff","Ship Staff Insp.","During abandon ship drill it was observed that in muster list ''STBD SIDE UPER DECK NEAR LIFEBOAT'' is designated as secondary muster station,however there was no marking ,stencil and imo symbol posted at the designated location.","LSA / FFA","ISM Related","Human Error","5.13","High","","","Designated location \"STBD SIDE UPPER DECK NEAR LIFEBOAT'' was stenciled as secondary muster station and imo symbol posted.","2019-11-14T23:59:35","","Completed","2019-09-14T23:59:35","No","No","No","Internal"]
[null,null,null,4454,null,"24_25/10/2019 2:37:18 PM","2019-09-20T23:59:35","Defect","Ship Staff","Ship Staff Insp.","One of the section of atmospheric condenser S/W outlet pipline is observed to have a pin hole.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","External Factors","10.32","Very High","","","A new pipe fabricated and fitted in place .","2019-10-06T23:59:35","","Completed","2019-09-30T23:59:35","No","No","No","Internal"]
[null,null,null,4455,null,"24_25/10/2019 2:40:07 PM","2019-09-25T23:59:35","Defect","Ship Staff","Ship Staff Insp.","OWS bilge inlet pipe observed having a hole at the welded connection.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Behaviour Based,External Factors","6.14","High","","","In place hot work repair work carried out.","2019-09-27T23:59:35","","Completed","2019-09-26T23:59:35","No","No","No","Internal"]
[null,null,null,4459,null,"24_25/10/2019 3:26:11 PM","2019-09-26T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ME L.O filter outlet valve flange leaking.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Valve gasket renewed. ","2019-10-22T23:59:35","","Completed","2019-10-15T23:59:35","No","No","No","Internal"]
[null,null,null,4407,null,"24_25/10/2019 3:39:44 PM","2019-10-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Port windalss winch lever spool piece worn out.","Deck - Mooring Machinery","Mooring","Equipment Related","9.2","Very High","","","Reapirs carried out. Working fine now.","2020-01-23T23:59:35","DBAU190173","Completed","2020-02-23T23:59:35","No","No","No","Internal"]
[null,null,null,4408,null,"24_25/10/2019 3:41:49 PM","2019-10-08T23:59:35","Defect","Ship Staff","Ship Staff Insp.","LO purifier heater is leaking and the solenoid valve block is defective.","E/R - Purifier","Eng. / Strg. Comp.","Equipment Related","10.2","Low","","","Heater renewed, solenoid valves overhauled. System working satisfactorily.","2020-01-23T23:59:35","DBAU190179","Completed","2020-02-26T23:59:35","No","No","No","Internal"]
[null,null,null,9572,null,"24_07/01/2020 1:42:54 PM","2019-10-11T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","The 3rd Officer was not familiar with the calibration procedure for the portable gas instrument.","Cargo Mach.","Cargo / Ballast Systems","Human Error","5.23","Very High","","","Training of the calibration of portable gas meters given to all ship staff.","2020-01-10T23:59:35","","Completed","2019-12-30T23:59:35","No","No","No","Internal"]
[null,null,null,9573,null,"24_07/01/2020 1:46:55 PM","2019-10-11T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","The record of comparison of the UTI temperate against the shore calibrated UTI was not available.","Cargo Mach.","Cert. & Docu.","Equipment Related","8.12","Medium","","","Others UTI's compared with shore calibrated UTI.","2020-01-10T23:59:35","","Completed","2019-12-30T23:59:35","No","No","No","Internal"]
[null,null,null,9574,null,"24_07/01/2020 1:52:23 PM","2019-10-11T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","The back up port side navigation light was not working.","Critical Equip.","Emgcy. Systems","Equipment Related","4.8","Medium","","","Navigation lights maintainence to be checked on regular basis. All navigation lights are in working condition. Test carried out on regular basis. ","2020-01-10T23:59:35","","Completed","2019-12-30T23:59:35","No","No","No","Internal"]
[null,null,null,8068,null,"24_Wed Jun 12 2019 01:02:47 GMT+0000 (Coordinated Universal Time)","2019-10-11T23:59:35","Defect","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","GRAB LINE OF THE ONE LIFEBUOY LOCATED ON THE PORT SIDE OF THE MAIN DECK NEAR MANIFOLD AREA WAS OBSERVED NOT ‘NON KINKING’ TYPE","LSA / FFA","Safety / LSA / FFA","Human Error","5.31","High","","","Vessel changed grab line of life buoy to NON KINKING type.","2019-11-21T23:59:35","","Completed","2019-10-13T23:59:35","No","No","No","External"]
[null,null,null,5709,null,"24_31/10/2019 1:10:49 PM","2019-10-21T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Aft draft gauge indicator on cargo console in CCR is shwoing incorrect reading","Miscellaneous","Cargo / Ballast Systems","Equipment Related","11.1","High","","","Purge air adjusted through blow off valve. The parameters of indicator also corrected. The indicator gauge is now showing same reading as SAAB computer, with very small error.","2019-11-21T23:59:35","","Completed","2019-11-11T23:59:35","No","No","No","Internal"]
[null,null,null,6023,null,"24_14/11/2019 7:21:47 PM","2019-11-05T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Brake band stopperbolt gap-found of various clearances","Deck - Mooring Machinery","Mooring","Equipment Related","9.7","Medium","","","Adjust as per maker reccommendation.","2019-11-26T23:59:35","","Completed","2019-11-10T23:59:35","No","No","No","Internal"]
[null,null,null,6024,null,"24_14/11/2019 7:22:59 PM","2019-11-05T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","all light fitting around accommodation block-bracket/angles rusted","Accommodation","General Appearance","Equipment Related","11.1","High","","","De rusting and painting completed.","2019-12-05T23:59:35","","Completed","2019-11-23T23:59:35","No","No","No","Internal"]
[null,null,null,6025,null,"24_15/11/2019 12:18:12 PM","2019-11-05T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Transfer line to slop tank, save drain found closed with nut/bolt arrangement.","Deck - Pipe / Fittings","Emgcy. Systems","Equipment Related","6.3","Low","","","Installed a proper plug and lashed.","2019-11-20T23:59:35","","Completed","2019-11-07T23:59:35","No","No","No","Internal"]
[null,null,null,6026,null,"24_15/11/2019 12:23:18 PM","2019-11-05T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","LSMGO Bunker Line - Isolation valves were normally butterfly valves.","Deck - Pipe / Fittings","MARPOL Related","Equipment Related","11.4","Very High","","","Valves renewed.","2020-01-22T23:59:35","","Completed","2020-03-21T23:59:35","No","No","No","Internal"]
[null,null,null,6027,null,"24_15/11/2019 12:26:56 PM","2019-11-05T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Few winch's operating platform angles found rusted / wasted","Deck - Mooring Machinery","Mooring","Equipment Related","11.5","Medium","","","New platform fabricated and in place. All other such platforms are in good condition.","2020-01-05T23:59:35","","Completed","2019-12-21T23:59:35","No","No","No","Internal"]
[null,null,null,6028,null,"24_15/11/2019 12:30:54 PM","2019-11-05T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","No.7 Foam monitor leaking from flange","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.38","High","","","Seal rings changedto rectify the leakage. ","2019-11-20T23:59:35","","Completed","2019-11-20T23:59:35","No","No","No","Internal"]
[null,null,null,6029,null,"24_15/11/2019 12:35:12 PM","2019-11-05T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Gangway - filter air / lubricators found seized and no indication of anyone ever checked - water was found full in drain chamber and no oil in lubricator chamber.","Miscellaneous","ISM Related","Equipment Related","5.47","Medium","","","Air filter, and lubricator renewed. Periodical draining and inspection carried out.","2019-11-12T23:59:35","","Completed","2019-11-17T23:59:35","No","No","No","Internal"]
[null,null,null,6030,null,"24_15/11/2019 12:38:03 PM","2019-11-05T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Hose crane - exterior/ boom/housing/hook blocks - rusty/dirty","Deck - Machinery","General Appearance","Equipment Related","11.3","Medium","","","Derusting and painting COMPLETED","2019-12-22T23:59:35","","Completed","2020-01-02T23:59:35","No","No","No","Internal"]
[null,null,null,6031,null,"24_15/11/2019 12:40:46 PM","2019-11-05T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","PV Breaker vent flange gasket damaged","Inert Gas","Cargo / Ballast Systems","Equipment Related","8.21","High","",""," included in REFMAN to attend in DD.","2019-11-15T23:59:35","","Completed","2019-11-17T23:59:35","Yes","No","No","Internal"]
[null,null,null,6032,null,"24_15/11/2019 12:43:58 PM","2019-11-05T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","VRCS- Additional drop valve cabinet on deck - observed oil leaks from valve housing, connections.","Cargo Mach.","MARPOL Related","Equipment Related","8.11","Medium","","","Temporary repair carried out. Job added in REFMAN for permamnet repair.","2019-11-25T23:59:35","","Completed","2019-11-09T23:59:35","No","No","No","Internal"]
[null,null,null,6033,null,"24_15/11/2019 1:25:59 PM","2019-11-05T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Scattered spot rust noticed on main deck and standing structures","Hull & Tanks","General Appearance","Equipment Related","11.3","Medium","","","Spot derusting and painting carried out. Cosmetic upgradation of main deck is always under progress.","2020-01-05T23:59:35","","Completed","2019-12-21T23:59:35","No","No","No","Internal"]
[null,null,null,6034,null,"24_15/11/2019 1:28:21 PM","2019-11-05T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Spring mooring winches - Exterior rusty /dirty","Deck - Mooring Machinery","Mooring","Equipment Related","11.5","Medium","","","Derusting and painting completed.","2019-12-22T23:59:35","","Completed","2019-12-30T23:59:35","No","No","No","Internal"]
[null,null,null,6035,null,"24_15/11/2019 1:31:38 PM","2019-11-05T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Fwd Fog horn - External look doesnot reveal that it was regularly checked for routines - though PMS is updated.","Navigation - Others","Navigation","Equipment Related","11.5","Medium","","","Fog horn operated every noon. The maintenance will be carried out releigiously as per the PMS, or as and when required. To begin with, initial cleaning done.","2019-12-01T23:59:35","","Completed","2019-11-21T23:59:35","No","No","No","Internal"]
[null,null,null,6036,null,"24_15/11/2019 1:35:56 PM","2019-11-05T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Main deck - Regular water washing regime recommended was not followed","Hull & Tanks","General Appearance","Equipment Related","11.3","Medium","","","Water washing regime implemented, washing done with deck fresh water at normal pressure. Hydroblaster is inoperational. Chemical used to remove the stains.","2019-11-05T23:59:35","","Completed","2019-11-06T23:59:35","No","No","No","Internal"]
[null,null,null,6037,null,"24_15/11/2019 1:59:55 PM","2019-11-05T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Job reporting in PMS to be done properly, enclosed with relevant forms and pictures.","Miscellaneous","Eng. / Strg. Comp.","Inappropriate Procedure","10.12","Very High","","","All Engineers and officers briefed.","2019-11-07T23:59:35","","Completed","2019-11-07T23:59:35","No","No","No","Internal"]
[null,null,null,6038,null,"24_15/11/2019 2:12:20 PM","2019-11-05T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Gas leak marks noticed on Aux boiler exhaust trunking","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Raised in REFMAN, RO will be raised for bellow.","2020-01-05T23:59:35","","Completed","2019-11-08T23:59:35","No","No","No","Internal"]
[null,null,null,6040,null,"24_15/11/2019 3:51:12 PM","2019-11-05T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","NO-01 economiser feed pump running,observed noise from motor bearing side.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Motor overhauled with new bearings. Observed no abnormal noise.","2019-11-21T23:59:35","","Completed","2019-11-09T23:59:35","No","No","No","Internal"]
[null,null,null,6041,null,"24_15/11/2019 3:56:32 PM","2019-11-05T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Elevator could hear cable touching noise/ or some other abnormal noise while travelling in the elevator.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","11.1","High","","","Checked and found all in good order. The travelling cable when collects, flappers to the cable tray due to sea way motion which gives some sound.","2019-11-21T23:59:35","","Completed","2019-11-11T23:59:35","No","No","No","Internal"]
[null,null,null,6042,null,"24_15/11/2019 4:02:19 PM","2019-11-05T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Old atmospheric condenser lying on funnel deck.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Old atmospheric condenser to offland for reconditioning in DD. The repair job has been added in REFMAN","2019-11-12T23:59:35","","Completed","2019-11-08T23:59:35","No","No","No","Internal"]
[null,null,null,6043,null,"24_15/11/2019 2:09:34 PM","2019-11-05T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","LO inlet temperature to purifier maintained at 87 Deg C","E/R - Purifier","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","To always maintain 95DegC","2019-11-07T23:59:35","","Completed","2019-11-06T23:59:35","No","No","No","Internal"]
[null,null,null,6044,null,"24_15/11/2019 2:15:13 PM","2019-11-05T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Aux boiler gauge glass showing different level with the adjacent one","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Gauge glass valves are open, blow through done, both are showing same level.","2019-11-07T23:59:35","","Completed","2019-11-06T23:59:35","No","No","No","Internal"]
[null,null,null,9568,null,"24_07/01/2020 1:54:56 PM","2019-11-07T23:59:35","Non Conformity","Ship Staff","Ship Staff Insp.","GARBAGE NOT SEGREGATED PROPERLY WHILE PUTTING THE GARBAGE INTO DESIGNATED DRUMS.","Miscellaneous","MARPOL Related","Human Error","6.2","High","","","IMMEDIATELY THAT CREW WAS STOPPED FROM PUTTING THE GARBAGE IN DRUM, CALLED UP AND GARBAGE SEGREGATION WAS EXPLAINED TO HIM.","2019-11-21T23:59:35","","Completed","2019-11-07T23:59:35","No","No","No","Internal"]
[null,null,null,8069,null,"24_Wed Jun 12 2019 01:07:03 GMT+0000 (Coordinated Universal Time)","2019-11-09T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Others (Eg. Insurance etc.)","12.20.05.011.04 - Pre Arrival and Commencement of Cargo Operations : \n\nTime of Completion of Checklist Not mentioned at Sec D. \n\n","Documentation","Cert. & Docu.","Human Error","5.9","Very High","","","Time of Completion of checklist completed. \n\nOfficers have been briefed to fill all data correctly and not to file the checklist without checking all the required data in checklist.\n\nPlease find attached scanned checklist.\n\n","2019-12-22T23:59:35","","Completed","2019-11-18T23:59:35","No","No","No","External"]
[null,null,null,8070,null,"24_Wed Jun 12 2019 01:09:35 GMT+0000 (Coordinated Universal Time)","2019-11-09T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Entries in CCR Movement Book :\n\nTime of Commencement of Ballasting at Dongjiakou not sighted in CCR Movement Look on 25 Oct 2019. \n\n","Documentation","Cert. & Docu.","Human Error","5.9","Very High","","","Entry has been made in CCR log.\n\nOfficers have been briefed to comply with Instructions for completing the CCR log given in starting pages of CCR Log.\n\nPlease find attached scanned pages of CCR Log.\n\n","2019-12-22T23:59:35","","Completed","2019-11-18T23:59:35","No","No","No","External"]
[null,null,null,8071,null,"24_Wed Jun 12 2019 01:12:01 GMT+0000 (Coordinated Universal Time)","2019-11-09T23:59:35","Defect","SIRE / CDI Insp.","Others (Eg. Insurance etc.)","Pre arrival tests and checks prior discharge operations at Dongjiakou - No evidence of tests and checks carried out on cargo and ballast hydraulic valves and VRCS.","Documentation","Cert. & Docu.","Human Error","8.11","Medium","","","Entry has been made in CCR log.\n\nOfficers have been briefed to comply with Instructions for completing the CCR log given in starting pages of CCR Log.\n\nPlease find attached scanned pages of CCR Log.\n\n","2019-12-22T23:59:35","","Completed","2019-11-18T23:59:35","No","No","No","External"]
[null,null,null,8072,null,"24_Wed Jun 12 2019 01:14:12 GMT+0000 (Coordinated Universal Time)","2019-11-09T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Bunkering Audit","Bunker Transfer Plan / Checklist 12.04.08.011.01 Section 7 - Monitoring of H2S/Benzene Vapors :  \n\nBenzene reading measured by detector tubes shall be mentioned < Min value that can be measured by the specific tube. For example by Gastec tubes Min measurable value is 0.05 ppm, hence in that case benzene shall be mention <0.05 ppm (if no discoloration observed)\n\nUnderstand vessel has kept the Gas tubes as evidence of monitoring.\n\n","Documentation","Cert. & Docu.","Human Error","10.5","Low","","","Space in section 7 is not sufficient to include all repetative checks, so an extra page has been added, with benezene ppm mentined less than min. value (which is 0.1). Vessel is retaining all the used gas tubes as an evidence.  ","2019-12-22T23:59:35","","Completed","2019-11-18T23:59:35","No","No","No","Internal"]
[null,null,null,8063,null,"24_30/11/2019 7:32:29 PM","2019-11-11T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Hydroblaster is non operational, the Nozzle and connecting piece required to be changed.","Deck - Machinery","General Appearance","Equipment Related","11.3","Medium","","","Repairs carried out. Nozzle renewed. Working satisfactorily now.","2020-01-22T23:59:35","DBAU190192","Completed","2020-02-28T23:59:35","No","No","No","Internal"]
[null,null,null,8073,null,"24_Thu Sep 12 2019 00:59:27 GMT+0000 (Coordinated Universal Time)","2019-11-28T23:59:35","Defect","Ship Staff","Ship Staff Insp.","M/E F.O. Supply pump No. 1 observed to have slight leakage through shaft seal.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Pump overhauled , bearing and mechanical seal changed. Leakage rectified.","2019-12-29T23:59:35","","Completed","2019-11-29T23:59:35","No","No","No","Internal"]
[null,null,null,9569,null,"24_07/01/2020 1:59:38 PM","2019-12-07T23:59:35","Non Conformity","Ship Staff","Ship Staff Insp.","One of the Bench Vice in Engine room workshop found broken, but it was still being used. Immediately do not use notice was displayed, and the vice was changed.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","1. Do not use notice displayed.\n\n2. Broken bench Vice removed and a new bench vice fitted in place.","2020-03-07T23:59:35","","Completed","2019-12-09T23:59:35","No","No","No","Internal"]
[null,null,null,9041,null,"24_24/12/2019 5:29:58 PM","2019-12-11T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Aft peak tank remote level gauge is showing erratic reading.","Hull & Tanks","Cargo / Ballast Systems","Equipment Related","8.12","Medium","","","Rectified by adjusting the purge air.","2020-03-10T23:59:35","","Completed","2019-12-27T23:59:35","No","No","No","Internal"]
[null,null,null,9042,null,"24_24/12/2019 7:08:48 PM","2019-12-13T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Slight leakage observed from the operating lever of mooring winch no. M 5. The lever is also hard to move.","Deck - Mooring Machinery","Mooring","Equipment Related","9.14","Medium","","","Operating lever block overhauled. Seals renewed. Test run carried out satisfactorily. working smooth and no leakage present now.","2020-03-12T23:59:35","DBAU190205","Completed","2020-03-10T23:59:35","No","No","No","Internal"]
[null,null,null,9551,null,"24_11/01/2020 9:40:53 AM","2019-12-28T23:59:35","Observation","Ship Staff","Ship Staff Insp.","All accommodation lights to change with LED lights","Accommodation ","General Appearance","Equipment Related,Industry Issue","11.13","Low","","","Detailed count forwarded to office. Work re-generated on 15 May 2020","2020-04-21T23:59:35","DBAU200007","Completed","2020-05-06T23:59:35","No","No","No","Internal"]
[null,null,null,9570,null,"24_07/01/2020 2:03:24 PM","2019-12-28T23:59:35","Non Conformity","Ship Staff","Ship Staff Insp.","Engine room switched off Tele motor (Steering system) no. 2 which was in use with out informing bridge, vessel was in open seas.\n\n","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Human Error","10.6","Very High","","","Duty officer was informed that Engineers is going to work on stand by steering gear motor (No.2), so the power will be switched off. The telemotor in use at that time was No. 2 , which was not communicated by the duty officer to duty engineer, and when the power for No. 2 steering motor was switched off, telemotor No. 2 also stopped. Realising this, duty Officer immediately changed over to No. 01 Tele motor (steering system) & Master informed about the situation. Both Duty officer and duty engineer were instructed to have proper exchange of information before going ahead for any such activities.","2020-03-28T23:59:35","","Completed","2019-12-28T23:59:35","No","No","No","Internal"]
[null,null,null,10394,null,"24_02/02/2020 8:07:38 AM","2020-01-18T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Emergency generator hydraulic start fails to pick up at first instance","Elect. Mach. & Equip.","Emgcy. Systems","Equipment Related","10.34","High","","","Dog and pinion renewed. tested satisfactorily.","2020-03-16T23:59:35","DBAU200045","Completed","2020-03-09T23:59:35","No","No","No","Internal"]
[null,null,null,10396,null,"24_02/02/2020 8:00:06 AM","2020-01-18T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Quick closing valve for incinerator waste oil tank inoperational","LSA / FFA","Emgcy. Systems","Equipment Related","10.17","Very High","","","Valve overhauled, new air line fabricated","2020-01-18T23:59:35","","Completed","2020-01-18T23:59:35","No","No","No","Internal"]
[null,null,null,10395,null,"24_02/02/2020 8:18:20 AM","2020-01-19T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Main engine unit-7 piston rings section found brocken ","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.4","High","","","Unit overhauled, liner renewed. rings renewed.","2020-02-06T23:59:35","","Completed","2020-01-26T23:59:35","No","No","No","Internal"]
[null,null,null,11008,null,"24_27/02/2020 4:46:24 PM","2020-02-05T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Stbd Lifeboat windshield reported leaking from sealing.","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.28","Very High","","","Packing replaced. Tested & found satisfactory","2020-02-24T23:59:35","","Completed","2020-02-15T23:59:35","No","No","No","Internal"]
[null,null,null,11009,null,"24_27/02/2020 3:03:26 PM","2020-02-05T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Accommodation block front rust weepings on port hole sills.","Accommodation","General Appearance","Equipment Related","11.8","Low","","","De-rusting & painting done. rust stains cleaned with rust remover. Target date revised due to job prioritization.","2020-05-05T23:59:35","","Completed","2020-05-05T23:59:35","No","No","No","Internal"]
[null,null,null,11010,null,"24_27/02/2020 4:52:08 PM","2020-02-05T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","VRCS Remote valve box corrosion at various levels.","Deck - Machinery","General Appearance","Equipment Related","11.4","Very High","","","Deck valve control boxes fwd to midship de-rusted and painted including channel. Target date revised due to job prioritization and trading pattern.","2020-05-11T23:59:35","","Completed","2020-05-03T23:59:35","No","No","No","Internal"]
[null,null,null,11011,null,"24_27/02/2020 2:59:22 PM","2020-02-05T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Pump room Blower Mesh sections disengaged from securing arrangements / damaged.","Deck - Machinery","General Appearance","Equipment Related","5.18","High","","","Mesh sections inspected and secured.","2020-02-20T23:59:35","","Completed","2020-02-11T23:59:35","No","No","No","Internal"]
[null,null,null,11012,null,"24_27/02/2020 4:56:42 PM","2020-02-05T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Few of the Manifold Gratings rusted / wasted.","Deck - Pipe / Fittings","General Appearance","Equipment Related","6.6","Medium","","","Necessary maintenance carried out and repainted.","2020-03-05T23:59:35","","Completed","2020-03-02T23:59:35","No","No","No","Internal"]
[null,null,null,11013,null,"24_27/02/2020 6:08:45 PM","2020-02-05T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Fwd Mast wires - dry, no evidence of greasing","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.8","Low","","","Greasing carried out.","2020-02-20T23:59:35","","Completed","2020-02-16T23:59:35","No","No","No","Internal"]
[null,null,null,11014,null,"24_27/02/2020 6:19:10 PM","2020-02-05T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Few foam Monitors Gratings rusty / corroded","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.35","Medium","","","All corroded gratings were derusted and repainted.","2020-03-05T23:59:35","","Completed","2020-03-03T23:59:35","No","No","No","Internal"]
[null,null,null,11015,null,"24_27/02/2020 6:21:33 PM","2020-02-05T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Mooring Winch / Windlass operating platform gratings found corroded / wasted.","Deck - Mooring Machinery","Mooring","Equipment Related","9.2","Very High","","","Wasted section of gratings replaced with onboard spare gratings.","2020-03-20T23:59:35","","Completed","2020-03-11T23:59:35","No","No","No","Internal"]
[null,null,null,11016,null,"24_27/02/2020 6:34:41 PM","2020-02-05T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Fwd Fog Horn - Motor exterior in bad shape, horn cone section also not in good shape.","Navigation - Others","Navigation","Equipment Related","12.12","High","","","Target date extended, awaiting suitable conditions and other jobs prioritization. Motor inspected, insulation tested. found in good and healthy condition. Horn tested and is working satisfactorily.Other PMS jobs carried out. Cosmetic maintenance of motor and cone carried out.","2020-03-05T23:59:35","","Completed","2020-02-24T23:59:35","No","No","No","Internal"]
[null,null,null,11017,null,"24_28/02/2020 6:02:43 PM","2020-02-05T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Intermediate shaft pedestal leakage","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","To attempt in dry dock, refman reference BA/SDR/1-ENG.37","2020-02-20T23:59:35","","Completed","2020-02-19T23:59:35","Yes","No","No","Internal","if REFFMAN defect made, Pls close the defect"]
[null,null,null,11018,null,"24_27/02/2020 6:27:28 PM","2020-02-05T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Fwd Store exterior dirty / with rust weepings.","Miscellaneous","General Appearance","Equipment Related","11.8","Low","","","Washed, De-rusted & painted. Target date revised due to job prioritization.","2020-03-20T23:59:35","","Completed","2020-03-01T23:59:35","No","No","No","Internal"]
[null,null,null,11019,null,"24_28/02/2020 6:16:40 PM","2020-02-05T23:59:35","Defect,Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Elevator cage is not aligning with landing platform","Accommodation","MLC Related","Equipment Related","11.16","Low","","","Target date revised due to job requiring shore attendance. Service done by shore technicians. ","2020-04-21T23:59:35","","Completed","2020-03-28T23:59:35","No","No","No","Internal"]
[null,null,null,11025,null,"24_27/02/2020 6:29:45 PM","2020-02-05T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","fwd Store stbd side ceiling has dark spray spot scattered.","Miscellaneous","General Appearance","Equipment Related","11.8","Low","","","Target date extented as awaiting suitable opportunity as job prioritized and planned for a rainy weather day. Ceiling dark spot painted over. ","2020-05-05T23:59:35","","Completed","2020-04-29T23:59:35","No","No","No","Internal","This can be done in stages - area wise - do not transfer to DD and carry out whenever feasible.\nIf any defect transferred to DD/REFFMAN then close it."]
[null,null,null,11026,null,"24_27/02/2020 3:07:06 PM","2020-02-05T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","mooring Winch M4 control valve block leaking.","Deck - Mooring Machinery","Mooring","Equipment Related","9.5","High","","","valve block replaced with spares.","2020-02-12T23:59:35","","Completed","2020-02-11T23:59:35","No","No","No","Internal"]
[null,null,null,11027,null,"24_27/02/2020 4:04:45 PM","2020-02-05T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Accommodation gangway - Wire reel box oil renewal due.","Miscellaneous","Safety / LSA / FFA","Equipment Related","5.47","Medium","","","Gear Oil changed of Accommodation gangway motors.","2020-03-05T23:59:35","","Completed","2020-02-16T23:59:35","No","No","No","Internal"]
[null,null,null,11028,null,"24_27/02/2020 4:27:17 PM","2020-02-05T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","PV breaker Top Mushroom Flange fully rusted & corroded.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.41","Medium","","","De rusting & painting carried out.","2020-02-20T23:59:35","","Completed","2020-02-18T23:59:35","No","No","No","Internal"]
[null,null,null,11029,null,"24_28/02/2020 6:05:35 PM","2020-02-05T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Service air compressor air filter found dirty","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Filter renewed","2020-02-20T23:59:35","","Completed","2020-02-06T23:59:35","No","No","No","Internal"]
[null,null,null,11030,null,"24_28/02/2020 6:21:05 PM","2020-02-05T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Area behind LSMGO chiller dirty","Miscellaneous","General Appearance","Human Error","11.1","High","","","Cleaned and painted","2020-02-20T23:59:35","","Completed","2020-02-08T23:59:35","No","No","No","Internal"]
[null,null,null,11031,null,"24_28/02/2020 6:25:35 PM","2020-02-05T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Main engine unit 5&7 leak off collecting funnel have fuel stains","E/R - Main Engine","Eng. / Strg. Comp.","Human Error","10.32","Very High","","","Funnel cleaned and painted","2020-02-20T23:59:35","","Completed","2020-02-12T23:59:35","No","No","No","Internal"]
[null,null,null,11032,null,"24_28/02/2020 6:30:08 PM","2020-02-05T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","A few tube/LED diffuserrs have hair line cracks","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","11.9","Low","","","Diffusers renewed","2020-02-20T23:59:35","","Completed","2020-02-13T23:59:35","No","No","No","Internal"]
[null,null,null,11033,null,"24_28/02/2020 6:32:25 PM","2020-02-05T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Light near no. 2 IG blower fused","Documentation,Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","11.9","Low","","","Light renewed","2020-02-06T23:59:35","","Completed","2020-02-06T23:59:35","No","No","No","Internal"]
[null,null,null,11034,null,"24_27/02/2020 6:24:03 PM","2020-02-05T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Port Windlass brake wheel stopper nut locking sheared off, hampering braking arrangements.","Deck - Mooring Machinery","Mooring","Equipment Related","9.2","Very High","","","Stopper nut Overhauled.","2020-02-20T23:59:35","","Completed","2020-02-19T23:59:35","No","No","No","Internal"]
[null,null,null,11035,null,"24_27/02/2020 4:01:07 PM","2020-02-05T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Cow Line near root valve 5C TC084, Oil streaks from rust spot on Line","Deck - Pipe / Fittings","MARPOL Related","Equipment Related","8.34","High","","","Chipped and painted COW Line near 5C Root Valve TC 084, found Line in good condition.","2020-03-05T23:59:35","","Completed","2020-02-17T23:59:35","No","No","No","Internal"]
[null,null,null,11036,null,"24_27/02/2020 6:31:50 PM","2020-02-05T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Life rafts cradle found rusted and devoid of maintenance.","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.28","Very High","","","De-rusted & painted","2020-03-05T23:59:35","","Completed","2020-02-24T23:59:35","No","No","No","Internal"]
[null,null,null,11037,null,"24_27/02/2020 2:29:06 PM","2020-02-05T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Dish washer Not working","Miscellaneous","MLC Related","Equipment Related","11.16","Low","","","Repairs done, equipment is in working condition","2020-04-05T23:59:35","","Completed","2020-03-13T23:59:35","No","No","No","Internal"]
[null,null,null,11038,null,"24_28/02/2020 6:14:13 PM","2020-02-05T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Engine room FWD(s) bilge well noticed oil sheen on top","Hull & Tanks","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","ER all bilge wells cleaned ( required area painted)","2020-02-20T23:59:35","","Completed","2020-02-19T23:59:35","No","No","No","Internal"]
[null,null,null,17473,null,"24_17/01/2021 2:49:40 PM","2020-02-05T23:59:35","Other","Ship Staff","Ship Staff Insp.","ME Alpha lubricator pump station - Thermostat valve ","E/R - Aux. Mach.","Eng. / Strg. Comp.","Human Error","10.32","Very High","","","To check if the thermostat valve was replaced – 5 yearly routine as per maker, raise RO if not done - vessel has spare thermostat valve , routine to be done during 5 yearly service in dock.","2020-02-20T23:59:35","","Completed","2020-02-06T23:59:35","No","No","No","Internal"]
[null,null,null,17474,null,"24_17/01/2021 2:52:18 PM","2020-02-05T23:59:35","Other","Ship Staff","Suptd. Insp.","ME alpha lubricator pump station","E/R - Aux. Mach.","Eng. / Strg. Comp.","Behaviour Based,Human Error","10.32","Very High","","","Pump coupling- Could not witness, spare spider coupling kept next to pump – if not vailable as spare, to raise RO - spare coumpling spider available kept near the pump.","2020-02-20T23:59:35","","Completed","2020-02-06T23:59:35","No","No","No","Internal"]
[null,null,null,11004,null,"24_27/02/2020 4:42:32 PM","2020-02-05T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","cascade tank vent on deck, pipe section fully rusted and dirty.","Miscellaneous","General Appearance","Equipment Related","11.7","High","","","Pipe chipped/de-rusted and painted. ","2020-02-20T23:59:35","","Completed","2020-02-15T23:59:35","No","No","No","Internal"]
[null,null,null,11005,null,"24_27/02/2020 2:24:55 PM","2020-02-05T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Galley Big fridge not working","Accommodation,Miscellaneous","MLC Related","Equipment Related","11.16","Low","","","Old fridge removed from the galley and replaced with spare fridge. Tested working satisfactory. ","2020-03-05T23:59:35","","Completed","2020-02-27T23:59:35","No","No","No","Internal"]
[null,null,null,11006,null,"24_27/02/2020 4:24:27 PM","2020-02-05T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","foam Monitors - few turret springs in rusted condition","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.35","Medium","","","Checked and replaced turret springs","2020-02-20T23:59:35","","Completed","2020-02-15T23:59:35","No","No","No","Internal"]
[null,null,null,11007,null,"24_27/02/2020 4:38:51 PM","2020-02-05T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Port Provision Crane - Abnormal Squeaking Noise from luffing bearing while in operation","Deck - Machinery","Safety / LSA / FFA","Equipment Related","8.41","Medium","","","Greasing done while crane in motion, No noise is present currently. Will observe for some more occations before closing the defect. Job to be  transfered to refman as per Supt'd advise.","2020-02-12T23:59:35","","Completed","2020-02-11T23:59:35","Yes","No","No","Internal","Pls transfer defect to REFFMAN and close the defect."]
[null,null,null,11040,null,"24_27/02/2020 6:39:45 PM","2020-02-12T23:59:35","Non Conformity","Ship Staff","Ship Staff Insp.","2 Self igniting Lights of Life buoys found not working.","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.31","High","","","S. I Lights changed of both life buoys.","2020-02-20T23:59:35","","Completed","2020-02-12T23:59:35","No","No","No","Internal"]
[null,null,null,11039,null,"24_02/03/2020 5:01:37 AM","2020-02-16T23:59:35","Defect","Ship Staff","Ship Staff Insp.","A/C -1 ELE MOTOR WINDING DAMAGE","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","11.9","Low","","","MOTOR RENEWED","2020-02-20T23:59:35","","Completed","2020-02-20T23:59:35","No","No","No","Internal"]
[null,null,null,11022,null,"24_14/03/2020 10:12:52 AM","2020-03-02T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Port Provision crane access rungs found rusted","Deck - Machinery","General Appearance","Equipment Related","10.28","Low","","","Access rungs de-rusted & painted.","2020-05-06T23:59:35","","Completed","2020-04-19T23:59:35","No","No","No","Internal"]
[null,null,null,11023,null,"24_14/03/2020 10:17:01 AM","2020-03-02T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Stbd provision Crane access rungs found rusted","Deck - Machinery","General Appearance","Equipment Related","10.28","Low","","","Access rungs de-rusted & painted","2020-05-06T23:59:35","","Completed","2020-04-19T23:59:35","No","No","No","Internal"]
[null,null,null,11024,null,"24_14/03/2020 10:24:38 AM","2020-03-02T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Radar Mast Platform found rusted","Accommodation","General Appearance","External Factors","11.8","Low","","","De-rusting & painting carried out","2020-08-02T23:59:35","","Completed","2020-06-01T23:59:35","No","No","No","Internal"]
[null,null,null,11660,null,"24_21/04/2020 1:45:13 PM","2020-03-29T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Old brands of lube oil (CALTEX, FUCHS) are still present onboard","Miscellaneous","Eng. / Strg. Comp.","Inappropriate Procedure","11.8","Low","","","Inspected, Old brand are low BN 40 & 20 cylinder oils. and can't be consumed at present. 40 BN will be transfered to the tank as it get empty.","2020-06-28T23:59:35","","Completed","2020-06-05T23:59:35","No","No","No","Internal"]
[null,null,null,11661,null,"24_21/04/2020 1:51:00 PM","2020-03-29T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","A few lube oil drums in steering gear looks too old","Miscellaneous","Eng. / Strg. Comp.","Human Error","11.8","Low","","","Inspected, oil transfered to new drums, old ones discarded, rust removed from some drums and paint applied on top portion","2020-05-29T23:59:35","","Completed","2020-05-06T23:59:35","No","No","No","Internal"]
[null,null,null,11663,null,"24_23/04/2020 2:02:22 PM","2020-03-29T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","E/R vent fan suction filter structure is detached, some blowers do not have filter frames","E/R - Pipes/ valves & fittings","Structural Condn. / WT integrity ","Equipment Related","11.8","Low","","","Inspection carried out, filter frames are retro fitted structures, since the suction is too strong, suction filter will not work efficiently at the location.plan to remove the rest of the frames at convenient opportunity.","2020-05-25T23:59:35","","Completed","2020-05-25T23:59:35","No","No","No","Internal"]
[null,null,null,11664,null,"24_27/04/2020 10:09:39 PM","2020-03-29T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","VRCS - Hydraulic oil leak observed in valve box (BA 411 / BA 412).","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.11","Medium","","","Maintenance completed. no leaks existing at present","2020-04-28T23:59:35","","Completed","2020-04-28T23:59:35","No","No","No","Internal"]
[null,null,null,11666,null,"24_27/04/2020 10:22:18 PM","2020-03-29T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Fire Wire Reel fully rusted, brake / drum band rusted","Deck - Machinery","Mooring","Equipment Related","10.28","Low","","","De-rusted & painting carried out.","2020-05-22T23:59:35","","Completed","2020-05-20T23:59:35","No","No","No","Internal"]
[null,null,null,11667,null,"24_27/04/2020 10:26:22 PM","2020-03-29T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Coamings of WBT Tank domes observed under various stages of corrosion. ","Deck - Pipe / Fittings","General Appearance","Equipment Related","10.28","Low","","","2 - 5 P/S WBT de-rusted and painted. Refer report in Weekly maintenance report additionally.","2020-05-29T23:59:35","","Completed","2020-05-28T23:59:35","No","No","No","Internal"]
[null,null,null,11668,null,"24_27/04/2020 10:33:29 PM","2020-03-29T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","M5 Mooring Winch hydraulic Line U-clamps observed missing","Deck - Machinery,Deck - Mooring Machinery","Mooring","Equipment Related","9.14","Medium","","","U-clamp installed","2020-04-28T23:59:35","","Completed","2020-04-25T23:59:35","No","No","No","Internal"]
[null,null,null,11671,null,"24_27/04/2020 9:56:18 PM","2020-03-29T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","VRCS Hydraulic Valve boxes on deck packing channels corroded and rust weeping marks observed","Cargo Mach.","General Appearance","Equipment Related","10.28","Low","","","De-rusting & painting of VRCS boxes (including channel packing) completed.","2020-05-29T23:59:35","","Completed","2020-05-05T23:59:35","No","No","No","Internal"]
[null,null,null,11672,null,"24_23/04/2020 1:28:15 PM","2020-03-29T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Observed Oil presence on ME fuel valve test room","Miscellaneous","General Appearance","Inappropriate Procedure","11.8","Low","","","Oil cleaned, Equipment secured","2020-04-05T23:59:35","","Completed","2020-03-30T23:59:35","No","No","No","Internal"]
[null,null,null,11673,null,"24_23/04/2020 1:32:52 PM","2020-03-29T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Aux engine 3 Oil max filter pump not operational","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Filter pump renewed. System working satisfactorily.","2020-04-30T23:59:35","","Completed","2020-04-03T23:59:35","No","No","No","Internal"]
[null,null,null,11674,null,"24_23/04/2020 1:40:13 PM","2020-03-29T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Aft ICCP ( PSU) lamp indicator switch is held with insulation tape","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Switch renewed.","2020-04-05T23:59:35","","Completed","2020-04-03T23:59:35","No","No","No","Internal"]
[null,null,null,11675,null,"24_21/04/2020 1:37:10 PM","2020-03-29T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Control air drier not efficient. No much difference between inlet and outlet air temperatures.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Inspection carried out, radiator cleaned.  Control air drier for main engine is working fine with temperature difference of 10 deg. Control air drier re-generating filter for rest of the machinery operation is satisfactory","2020-04-23T23:59:35","","Completed","2020-04-15T23:59:35","No","No","No","Internal"]
[null,null,null,11676,null,"24_21/04/2020 1:31:46 PM","2020-03-29T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ECR A/C unit top corroted, condensation water collected on top","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Complete duct derusted and chipped, painting work completed","2020-04-28T23:59:35","","Completed","2020-04-20T23:59:35","No","No","No","Internal"]
[null,null,null,11677,null,"24_27/04/2020 10:29:33 PM","2020-03-29T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Few Areas on Main deck had paint cracks - indicating insufficient surface preparation","Hull & Tanks","General Appearance","Behaviour Based","10.28","Low","","","Wire brushed and painted after proper surface preparation done. Job supervised by C/O","2020-04-28T23:59:35","","Completed","2020-04-21T23:59:35","No","No","No","Internal"]
[null,null,null,11678,null,"24_23/04/2020 1:44:31 PM","2020-03-29T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Area under main engine turning observed with oil presence/leak. ","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Area cleaned and painted on 24 April. No fresh leak observed after sailing for 3 days","2020-04-28T23:59:35","","Completed","2020-04-18T23:59:35","No","No","No","Internal"]
[null,null,null,11679,null,"24_23/04/2020 1:55:54 PM","2020-03-29T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Foam room floor mats looks dirty.","Elect. Mach. & Equip.","General Appearance","Human Error","11.3","Medium","","","Mats washed , dried.","2020-04-09T23:59:35","","Completed","2020-04-06T23:59:35","No","No","No","Internal"]
[null,null,null,11682,null,"24_23/04/2020 1:51:47 PM","2020-03-29T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Elevator wires appears too dry","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Applied grease after taking all precautions.","2020-04-21T23:59:35","","Completed","2020-04-15T23:59:35","No","No","No","Internal"]
[null,null,null,11680,null,"24_11/04/2020 11:57:44 AM","2020-03-30T23:59:35","Defect","Ship Staff","Bunkering Audit","No-2 ( S) bunker tank filling valve actuator gear damaged while operating","Hull & Tanks","MARPOL Related","Equipment Related","6.7","High","","","Exchanged the gear with Diesel oil line valve actuator. DO line filling valve renewed","2020-05-30T23:59:35","","Completed","2020-04-05T23:59:35","No","No","No","Internal"]
[null,null,null,11681,null,"24_21/04/2020 7:05:22 AM","2020-04-03T23:59:35","Defect","Ship Staff","Ship Staff Insp.","A/C compressor-1 coupling damaged","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Coupling replaced with spare plates. New coupling plates ordered.","2020-04-06T23:59:35","","Completed","2020-04-04T23:59:35","No","No","No","Internal"]
[null,null,null,11665,null,"24_27/04/2020 10:14:48 PM","2020-04-30T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","COW Machines fitted with old drive unit from Maker","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.34","High","","","Replacement of COW Machine external drive unit. New unit received at Singapore - 42 nos. Completed - 42 nos / Pending - 0 nos. ","2020-07-31T23:59:35","","Completed","2020-05-14T23:59:35","No","No","No","Internal"]
[null,null,null,5708,null,"24_29/10/2019 3:51:35 PM","2020-05-05T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Inadequate inventory management of operational critical spares in PAL.","Miscellaneous","ISM Related","Behaviour Based,Human Error","10.12","Very High","","","All practical means of inventory are completed and updated in PAL.","2020-08-06T23:59:35","","Completed","2020-06-18T23:59:35","No","No","No","External"]
[null,null,null,11669,null,"24_27/04/2020 10:36:44 PM","2020-05-05T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","A-deck stbd deck drain pipe to main deck suspected holed and leaking","Deck - Pipe / Fittings","General Appearance","Equipment Related","10.28","Low","","","Job DK 24 has been added to REFMAN for crop/renew holed scupper pipe","2020-10-21T23:59:35","","Completed","2020-10-16T23:59:35","Yes","No","No","Internal","This can be attempted now, why defer to DD?\n\nIf defered to DD/REFFMAN made, then close the defect"]
[null,null,null,6039,null,"24_15/11/2019 2:17:31 PM","2020-05-05T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Spare inventory not properly updated in PAL","Miscellaneous","ISM Related","Behaviour Based,Human Error","10.13","Very High","","","All practical deck & engine  inventory is complete and updated in PAL","2020-08-06T23:59:35","","Completed","2020-06-18T23:59:35","No","No","No","Internal"]
[null,null,null,12028,null,"24_25/05/2020 2:07:19 PM","2020-05-06T23:59:35","Other","Owner / Marine / Tech. Suptd.","Engineering Audit","Conversion of fluorescent lights in to LED lights not complete and not done with circuit modification","Miscellaneous","General Appearance","Industry Issue","10.15","Low","","","circuit modification of 100 % fittings completed and converted to LED as on 27.02.2021 except for smaller tubelights for bathroom and bed lights which were not in original work scope. ","2021-02-19T23:59:35","DBAU200206, DBAU210037","Completed","2021-02-18T23:59:35","No","No","No","Internal"]
[null,null,null,12029,null,"24_01/06/2020 7:33:13 PM","2020-05-06T23:59:35","Defect","Ship Staff","Ship Staff Insp.","ME unit-3 X-head aft temperature sensor shows irregular readings occationally","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Sensor renewed (as repeated wrong readings appeared). working satisfactorily.","2020-06-06T23:59:35","","Completed","2020-06-06T23:59:35","No","No","No","Internal","Pls close this defect, if found normal or raise RO if any spares reqd"]
[null,null,null,12032,null,"24_25/05/2020 1:34:32 PM","2020-05-07T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Bunkering Audit","While verifying the bunker check list as part of audit, observed the\" benzene\" test reading entered wrongly as \" Zero\" insted of the value as < 0.1 PPM","Documentation","Cert. & Docu.","Human Error","2.5","Medium","","","Corrected the entry, changed it as <0.1 ppm , counter signed the column.","2020-05-13T23:59:35","","Completed","2020-05-13T23:59:35","No","No","No","Internal"]
[null,null,null,12030,null,"24_25/05/2020 2:12:32 PM","2020-05-14T23:59:35","Breakdown","Ship Staff","Engineering Audit","Engine room fan -4 ( port-aft), motor damaged","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Motor renewed. working satisfactorily","2020-06-14T23:59:35","","Completed","2020-06-21T23:59:35","No","No","No","Internal"]
[null,null,null,12033,null,"24_01/06/2020 7:39:55 PM","2020-05-21T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Main sea water pup-2 seal cooling line damage","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Cooling line renewed.","2020-05-27T23:59:35","","Completed","2020-05-22T23:59:35","No","No","No","Internal"]
[null,null,null,11662,null,"24_23/04/2020 1:49:16 PM","2020-05-29T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Observed the e/r hydraulic pump unit taking long time to build pressure during ME liner renewal.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","RO raised. DBAU 200114 -received new pump.","2020-09-06T23:59:35","DBAU200114","Completed","2020-09-04T23:59:35","No","No","No","Internal"]
[null,null,null,11670,null,"24_19/04/2020 2:46:07 PM","2020-06-05T23:59:35","Defect","Ship Staff","Ship Staff Insp.","AE#2 LO Priming motor tripping due to misalignment with pump","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","RO 200118 - motor and pump received - kept as standby. the existing one in use working well since last repairs","2020-09-21T23:59:35","","Completed","2020-09-11T23:59:35","No","No","No","Internal"]
[null,null,null,12031,null,"24_01/06/2020 7:27:55 PM","2020-06-19T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Main Engine unit-5 Crankpin bearing high temperature alarm appearing occationally","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Thorough inspection carried out. no hot spot or irregularity observed.  Sensor was faulty ( temp veries up and down). same replaced with new one.","2020-09-19T23:59:35","","Completed","2020-09-19T23:59:35","No","No","No","Internal"]
[null,null,null,11020,null,"24_14/03/2020 9:59:50 AM","2020-07-02T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Renewal of Port Hose Handling Crane top platform grating","Deck - Machinery","General Appearance","Equipment Related","8.5","Very High","","","Platform grating renewed by installing new grating.","2021-01-02T23:59:35","DBAU200076","Completed","2020-12-19T23:59:35","No","No","No","Internal"]
[null,null,null,11021,null,"24_14/03/2020 10:03:51 AM","2020-07-02T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Renewal of Stbd Hose Handling crane top platform grating","Deck - Machinery","General Appearance","Equipment Related","8.5","Very High","","","Platform grating renewed by installing new grating.","2021-01-02T23:59:35","DBAU200076","Completed","2020-12-19T23:59:35","No","No","No","Internal"]
[null,null,null,13253,null,"24_29/07/2020 2:35:35 PM","2020-07-19T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Steering gear grease pump relay defective","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Grease pump operational in manual mode. RO raised, 200161 - received - RECTIFIED WORKING SATISFACTORILY","2020-11-19T23:59:35","RO 200161","Completed","2020-09-26T23:59:35","No","No","No","Internal"]
[null,null,null,13254,null,"24_31/07/2020 4:04:19 PM","2020-07-21T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Engine room crane cable, loss of continuity","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Human Error","4.1","High","","","Wire section renewed. New cable received and standby for use if required.","2020-09-06T23:59:35","RO 200162","Completed","2020-09-04T23:59:35","No","No","No","Internal"]
[null,null,null,13446,null,"24_14/08/2020 12:48:23 PM","2020-07-25T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Pre-departure checklist older version in use","Documentation","ISM Related","Human Error","10.1","Medium","","","briefed the staff about the latest version checklists and from where to locate in the QDMS. All older version filled checklists replaced with new ones in the file.","2020-07-26T23:59:35","","Completed","2020-07-25T23:59:35","No","No","No","Internal"]
[null,null,null,13447,null,"24_15/08/2020 1:12:08 AM","2020-07-26T23:59:35","Defect","Ship Staff","Ship Staff Insp.","1S, 4P & 5C PV Valves were observed to be leaking badly with less pressure inside cargo tanks.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.21","High","","","1S, 4P & 5C PV Valves were overhauled and lapping carried out as per maker's procedure and leak arrested.","2020-07-31T23:59:35","","Completed","2020-08-01T23:59:35","No","No","No","Internal"]
[null,null,null,13448,null,"24_15/08/2020 2:34:32 PM","2020-07-26T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Valve indicator lamps in CCR panel for 6 nos cargo/ballast valves not working.","Cargo Mach.","Cargo / Ballast Systems","Inappropriate Procedure","11.1","High","","","All 6 nos valve indicators bulbs were renewed","2020-08-03T23:59:35","","Completed","2020-07-29T23:59:35","No","No","No","Internal"]
[null,null,null,13449,null,"24_15/08/2020 8:06:18 AM","2020-07-27T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Both wilden pumps not effectively bonded to the vessel's structure due to heavy paint/rust.","Critical Equip.,Deck - Pipe / Fittings","Cargo / Ballast Systems","Inappropriate Procedure","6.3","Low","","","Bonding cable area buffed to enable contact with the ship's structure","2020-08-03T23:59:35","","Completed","2020-08-01T23:59:35","No","No","No","Internal"]
[null,null,null,13450,null,"24_15/08/2020 8:14:09 AM","2020-07-27T23:59:35","Defect","Ship Staff","Ship Staff Insp.","IG O2 sampling pipe fwd of deck seal partly choked and small pipe section corroded.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.2","Medium","","","Pipe section removed, cleared and section fitted back after derusting and painting","2020-08-05T23:59:35","","Completed","2020-08-03T23:59:35","No","No","No","Internal"]
[null,null,null,13451,null,"24_15/08/2020 8:19:32 AM","2020-07-27T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Weathertight inspection doors of both hose handling cranes were found frozen.","Deck - Machinery","Cargo / Ballast Systems","Behaviour Based,Inappropriate Procedure","8.5","Very High","","","Both doors eased up and lubricated.","2020-08-06T23:59:35","","Completed","2020-07-29T23:59:35","No","No","No","Internal"]
[null,null,null,13452,null,"24_15/08/2020 11:38:32 AM","2020-07-27T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Stbd side pumproom blower fire flap unable to be kept in shut position in an emergency as the wire for the pin is coming in way of the securing toggle pin.","Cargo Mach.","Cargo / Ballast Systems","Human Error,Inappropriate Procedure","5.18","High","","","Toggle pin securing arrangement shifted to enable securing of pin to hold flap in shut position.","2020-08-06T23:59:35","","Completed","2020-07-29T23:59:35","No","No","No","Internal"]
[null,null,null,13453,null,"24_14/08/2020 12:29:19 PM","2020-07-28T23:59:35","Defect","Ship Staff","Ship Staff Insp.","ME unit 1 & 2 fuel pumps shock absorbers noted not operational and with leakage","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Unit 1 fuel pump shock absorber renewed and unit 2 fuel pump shock absorber replaced with overhauled one.","2020-08-05T23:59:35","","Completed","2020-08-03T23:59:35","No","No","No","Internal"]
[null,null,null,13463,null,"24_15/08/2020 8:31:12 PM","2020-07-29T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Fwd bosun store mechanical vent flap stuck in open position and cannot be closed","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","Inappropriate Procedure","5.17","Very High","","","Vent flap holding lever freed up","2020-08-05T23:59:35","","Completed","2020-08-02T23:59:35","No","No","No","Internal"]
[null,null,null,13454,null,"24_15/08/2020 8:34:53 AM","2020-07-30T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Vapour leak observed from 2 nos bolts of CL349 drain to 3P COT and with oil stains.","Deck - Pipe / Fittings","Cargo / Ballast Systems","External Factors","8.18","High","","","Hole rethreaded and fitted with three nos new bolts and vapour leak arrested.","2020-08-06T23:59:35","","Completed","2020-08-04T23:59:35","No","No","No","Internal"]
[null,null,null,13455,null,"24_15/08/2020 12:28:00 PM","2020-07-30T23:59:35","Defect","Ship Staff","Ship Staff Insp.","PV breaker vent cock valve wheel broken and vent pipe choked and covered by paint","Deck - Pipe / Fittings","Cargo / Ballast Systems","Human Error,Inappropriate Procedure","8.28","Medium","","","New vent cock valve fitted and new vent pipe arrangement fitted","2020-08-08T23:59:35","","Completed","2020-08-06T23:59:35","No","No","No","Internal"]
[null,null,null,13456,null,"24_15/08/2020 9:20:02 PM","2020-07-30T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Port side lifeboat sprinkler valve connecting rod for valve activation from on/off operating lever was observed to be detached.","LSA / FFA","Safety / LSA / FFA","Behaviour Based,Equipment Related","5.28","Very High","","","Connecting rod fixed into place, sprinker valve tried out and valve operating smoothly.","2020-08-06T23:59:35","","Completed","2020-08-05T23:59:35","No","No","No","Internal"]
[null,null,null,13457,null,"24_15/08/2020 9:25:12 PM","2020-07-30T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Stbd side lifeboat sprinkler valve was found stuck in open position","LSA / FFA","Safety / LSA / FFA","Human Error,Inappropriate Procedure","5.28","Very High","","","Valve freed up and operation verified","2020-08-06T23:59:35","","Completed","2020-08-05T23:59:35","No","No","No","Internal"]
[null,null,null,13458,null,"24_15/08/2020 8:44:26 PM","2020-07-30T23:59:35","Defect","Ship Staff","Ship Staff Insp.","No.1 fire isolation valve found jammed.","LSA / FFA","Safety / LSA / FFA","Human Error,Inappropriate Procedure","5.35","Medium","","","Fire isolation valve lubrication carried out and eased up.","2020-08-03T23:59:35","","Completed","2020-08-03T23:59:35","No","No","No","Internal"]
[null,null,null,13459,null,"24_15/08/2020 8:57:58 PM","2020-07-30T23:59:35","Defect","Ship Staff","Ship Staff Insp.","One temperature gauge in manifold has turned greenish black and rest of the manifold gauges calibration to be carried out.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.13","Medium","","","All manifold temperature and pressure gauges calibration carried out. The greenish black glycerine emptied from the gauge for filling new.","2020-08-06T23:59:35","","Completed","2020-08-03T23:59:35","No","No","No","Internal"]
[null,null,null,13441,null,"24_14/08/2020 12:00:28 PM","2020-08-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Main engine turning gear remote controller defective / erratic operation","E/R - Main Engine,Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Remote wire connector repaired by soldering the broken wire connections.","2020-08-11T23:59:35","","Completed","2020-08-11T23:59:35","No","No","No","Internal"]
[null,null,null,13442,null,"24_15/08/2020 8:44:32 AM","2020-08-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Locking arrangement found broken for the following IG inlet valves : 1P,1C,1S,2S,3P,4C,5S,SL P. 4P & 5P locking plate also in bad condition.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Behaviour Based,Human Error,Inappropriate Procedure","8.2","Medium","","","New wire locking arrangement fabricated.","2020-08-08T23:59:35","","Completed","2020-08-08T23:59:35","No","No","No","Internal"]
[null,null,null,13443,null,"24_14/08/2020 12:14:39 PM","2020-08-02T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Galley hot plate - low insulation alarm","Accommodation,Elect. Mach. & Equip.","General Appearance","Equipment Related","10.38","Medium","","","two hot plates renewed, to renew the connecting cables - new cable received and replaced for one plate. replaced one more hotplate + switch+cable. Presently no low insulation anywhere in the equipment","2021-01-21T23:59:35","","Completed","2020-12-24T23:59:35","No","No","No","Internal"]
[null,null,null,13460,null,"24_14/08/2020 11:48:10 AM","2020-08-02T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","FWD mast flood light (LED) defective","Elect. Mach. & Equip.","General Appearance","Equipment Related","11.1","High","","","Flood light fixture (LED) found with water ingress and some of the leds burnt. Fixture replaced with sodium lamp flood light fixture (old). LED flood light was supplied under DBAU195061.","2020-08-03T23:59:35","","Completed","2020-08-02T23:59:35","No","No","No","Internal"]
[null,null,null,13461,null,"24_15/08/2020 9:31:01 PM","2020-08-02T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Air leak observed in port side lifboat high pressure air hose section between air bottle valve and four way manifold","LSA / FFA","Safety / LSA / FFA","Inappropriate Procedure","5.28","Very High","","","Leaking high pressure replaced with onboard spare","2020-08-03T23:59:35","","Completed","2020-08-03T23:59:35","No","No","No","Internal"]
[null,null,null,13637,null,"24_25/08/2020 12:06:46 PM","2020-08-03T23:59:35","Defect","Ship Staff","Ship Staff Insp.","OBSERVED THAT FEW CARGO IG BRANCH VALVE LOCKING ARRANGEMENT HAS WASTED AND PAD LOCK CAN NOT BE FITTED.","Inert Gas","Cargo / Ballast Systems","Equipment Related","8.2","Medium","","","New wire locking arrangement fabricated.","2020-09-01T23:59:35","","Completed","2020-08-08T23:59:35","No","No","No","Internal"]
[null,null,null,13462,null,"24_15/08/2020 8:38:09 PM","2020-08-03T23:59:35","Defect","Ship Staff","Ship Staff Insp.","FP tank stbd side vent side cover three bolts missing from one side","Deck - Pipe / Fittings","General Appearance","Human Error,Inappropriate Procedure","11.7","High","","","New bolts fitted to tighten and keep the cover in place","2020-08-10T23:59:35","","Completed","2020-08-05T23:59:35","No","No","No","Internal"]
[null,null,null,13464,null,"24_14/08/2020 12:20:25 PM","2020-08-04T23:59:35","Defect","Ship Staff","Ship Staff Insp.","AE no.3 JCW thermostatic valve defective","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Thermostatic Valve elements renewed.","2020-08-05T23:59:35","","Completed","2020-08-04T23:59:35","No","No","No","Internal"]
[null,null,null,13444,null,"24_16/08/2020 4:00:21 AM","2020-08-05T23:59:35","Defect","Ship Staff","Ship Staff Insp.","AE starting air bottle - filling valve from emergency air comp found jammed with spindle broken","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","removed valve for overhaul and made functional.","2020-08-07T23:59:35","","Completed","2020-08-07T23:59:35","No","No","No","Internal"]
[null,null,null,13465,null,"24_14/08/2020 12:23:19 PM","2020-08-05T23:59:35","Defect","Ship Staff","Ship Staff Insp.","EGB water feed pump no.1 leakage from mechanical seal","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","pump overhauled with new mechanical seal","2020-08-06T23:59:35","","Completed","2020-08-05T23:59:35","No","No","No","Internal"]
[null,null,null,13445,null,"24_16/08/2020 4:32:46 AM","2020-08-06T23:59:35","Critical Equipment","Ship Staff","Ship Staff Insp.","Emergency air compressor foundation vibration dampers in worn out condition.","Critical Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","RO DBAU200173 raised dated 27 Aug 2020 for new vibration dampers. new dampers received and changed.","2020-09-21T23:59:35","","Completed","2020-09-16T23:59:35","No","No","No","Internal"]
[null,null,null,13617,null,"24_28/08/2020 11:25:43 AM","2020-08-07T23:59:35","Defect","Ship Staff","Ship Staff Insp.","ER funnel casing door coaming found wasted and with holes.","Miscellaneous","General Appearance","Equipment Related","11.6","Medium","","","To plan for hotwork in place for repairs in DD","2021-03-11T23:59:35","","Completed","2021-01-06T23:59:35","Yes","No","No","Internal"]
[null,null,null,13638,null,"24_28/08/2020 11:38:11 AM","2020-08-10T23:59:35","Defect,Observation","Ship Staff","Ship Staff Insp.","FO bunker tanks elevated vent heads saveall drains choked with rust. ","Deck - Pipe / Fittings","General Appearance","Equipment Related,Human Error","6.9","Low","","","Cleared up all elevated savealls drain pipes leading to the savealls located on the deck.","2020-08-12T23:59:35","","Completed","2020-08-12T23:59:35","No","No","No","Internal"]
[null,null,null,13628,null,"24_01/09/2020 11:43:09 AM","2020-08-15T23:59:35","Defect","Ship Staff","Ship Staff Insp.","One no. GX2009 personal gas meter found not working.","Miscellaneous","Cargo / Ballast Systems","Equipment Related,Human Error","5.23","Very High","","","Vessel received new personal gas meter.","2020-11-21T23:59:35","DBAU200186","Completed","2020-11-02T23:59:35","No","No","No","Internal"]
[null,null,null,13619,null,"24_25/08/2020 12:10:30 PM","2020-08-16T23:59:35","Defect","Ship Staff","Ship Staff Insp.","OBSERVED THAT STBD ANCHOR BOW STOPPER IS NOT LOCKING COMPLETELY DUE TO TWIST IN ANCHOR CHAIN","Deck - Mooring Machinery","Mooring","Equipment Related","9.2","Very High","","","Anchor chain twist removed.","2020-12-21T23:59:35","","Completed","2020-12-06T23:59:35","No","No","No","Internal"]
[null,null,null,13620,null,"24_25/08/2020 2:29:06 PM","2020-08-16T23:59:35","Defect","Ship Staff","Ship Staff Insp.","OBSERVED CITADEL IRIDIUM PHONE IS NOT WORKING.","Miscellaneous","ISPS Related","Equipment Related","7.6","Medium","","","ETO checked the phone. Contacted IT support. Troubleshooting in progress. As per IT support, Mr. Kamlesh the SIM is not active and will be activated prior passing any HRA","2020-11-16T23:59:35","","Completed","2020-11-08T23:59:35","No","No","No","Internal"]
[null,null,null,13622,null,"24_25/08/2020 3:34:15 PM","2020-08-16T23:59:35","Observation","Ship Staff","Ship Staff Insp.","OBSERVED WATER INGRESS IN BOTH L/BOATS DURING RAINS. ","LSA / FFA","Safety / LSA / FFA","External Factors","5.29","High","","","Lifeboat fwd and main hatch packings renewed, observed water ingress due to misalignment of doors. Job DK 54 added to REFMAN for repairs in drydock.","2020-12-11T23:59:35","","Completed","2020-12-07T23:59:35","Yes","No","No","Internal"]
[null,null,null,13639,null,"24_25/08/2020 11:51:49 AM","2020-08-16T23:59:35","Observation","Ship Staff","Ship Staff Insp.","PORT AND STBD BRIDGE WING SPEED LOG REPEATER DIMMERS NO WORKING AT OPTIMUM LEVEL OF BRIGHTNESS","Navigation - Echo Sounder / Speed Log","Navigation","Equipment Related","4.7","High","","","Rectified the lcd connector, working satisfactory now ","2020-08-17T23:59:35","","Completed","2020-08-17T23:59:35","No","No","No","Internal"]
[null,null,null,13640,null,"24_25/08/2020 11:55:45 AM","2020-08-16T23:59:35","Observation","Ship Staff","Ship Staff Insp.","OBSERVED THAT PORT AND STBD SOUND RECEPTION SYSTEM SPEAKERS POWER IS NOT SUFFCIENT. ONE HAS TO CLIMB UP THE LADDER AND SPEAK IN ORDER TO GET HEARD INSIDE THE BRIDGE.","Navigation - Others","Navigation","Equipment Related","4.7","High","","","Checked and replaced the stbd side mike. The sensitivity is low as the mikes are located at height and one has to speak loudly.","2020-08-17T23:59:35","","Completed","2020-08-17T23:59:35","No","No","No","Internal"]
[null,null,null,13624,null,"24_26/08/2020 7:17:35 AM","2020-08-17T23:59:35","Defect,Observation","Ship Staff","Ship Staff Insp.","OBSERVED 1S,4P,5C COT PV VALVE VAPOUR HISSING OUT FROM PRESSURE SIDE.IG PRESSURE BEING 200-300mmWG ONLY.","Inert Gas","Cargo / Ballast Systems","Equipment Related","8.39","Medium","","","SHIP STAFF HAS DONE LAPPING OF SUBJECT PV VALVES BUT STILL ISSUE IS NOT FULLY RESOLVED. NOW PV VV LIFTING AT 900mmWG. Job added to REFMAN for complete overhaul in drydock.","2020-11-13T23:59:35","Job DK17 added to REFMAN","Completed","2020-11-13T23:59:35","Yes","No","No","Internal"]
[null,null,null,13625,null,"24_26/08/2020 7:20:44 AM","2020-08-17T23:59:35","Defect,Observation","Ship Staff","Ship Staff Insp.","OBSERVED SL-P AND SL-S VAPOUR HISSING OUT FROM VACUUM SIDE.","Inert Gas","Cargo / Ballast Systems","Equipment Related","8.39","Medium","","","SHIP STAFF TRIED LAPPING THE VACUUM DISC BUT STILL SOMETIMES VAPOUR SEEN HISING OUIT FROM VACUUM SIDE. Job added to REFMAN for complete overhaul in drydock.","2020-11-13T23:59:35","Job Dk17 added to REFMAN","Completed","2020-11-13T23:59:35","Yes","No","No","Internal"]
[null,null,null,13626,null,"24_26/08/2020 7:24:12 AM","2020-08-17T23:59:35","Observation","Ship Staff","Ship Staff Insp.","HYD OIL LEAK OBSERVED ON STBD ANCHOR WINDLASS OPERATING LEVER WHILE ANCHORING OPERATIONS. Clutch valve found stuck in pressed position.","Deck - Mooring Machinery","Mooring","External Factors","9.2","Very High","","","Clutch valve and control block overhauled and working satisfactorily, leaks were rectified.","2020-12-21T23:59:35","","Completed","2020-11-30T23:59:35","No","No","No","Internal"]
[null,null,null,13627,null,"24_26/08/2020 7:26:44 AM","2020-08-17T23:59:35","Observation","Ship Staff","Ship Staff Insp.","HYD OIL LEAK OBSERVED ON M7 WINCH ( POOP DECK) FROM RETURN LINE PIPE GOING TO OPERATING LEVER BLOCK.","Deck - Mooring Machinery","Mooring","Equipment Related,External Factors","9.14","Medium","","","Pipe removed and repaired.  ","2020-09-20T23:59:35","","Completed","2020-09-16T23:59:35","No","No","No","Internal"]
[null,null,null,13629,null,"24_26/08/2020 7:36:12 AM","2020-08-17T23:59:35","Defect,Observation","Ship Staff","Ship Staff Insp.","PORT AND STBD HOSE HANDLING CRANE & PP ROOM DAVIT FLOATING BLOCK HOOK SWIVEL IS FROZEN ADN NOT FREE. ","Deck - Machinery","Cargo / Ballast Systems","Behaviour Based,Human Error","10.28","Low","","","Both Hose Handling Cranes and Pumproom Davit Hook Swivels Made Free.","2020-09-13T23:59:35","","Completed","2020-08-29T23:59:35","No","No","No","Internal"]
[null,null,null,13630,null,"24_26/08/2020 2:45:52 AM","2020-08-17T23:59:35","Defect","Ship Staff","Ship Staff Insp.","DURING MONTHLY INSPECTION OBSERVED THAT 10 LIFEJACKET LIGHTS NOT WORKING .EXPIRY DATES OF THESE LIGHTS IS JAN-2021.","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.32","High","","","All defective lifejackets lights were replaced with newly received lights","2020-09-13T23:59:35","DBAU200126","Completed","2020-09-08T23:59:35","No","No","No","Internal"]
[null,null,null,13636,null,"24_26/08/2020 7:51:27 AM","2020-08-17T23:59:35","Defect,Observation","Ship Staff","Ship Staff Insp.","2 NOS OF FOAM MONITORS ON DECK WERE FOUND LEAKING.","LSA / FFA","Safety / LSA / FFA","Behaviour Based,Human Error","5.38","High","","","BOTH FOAM MONITORS OVERHAULED AND LEAK RECTIFIED.","2020-09-09T23:59:35","","Completed","2020-08-29T23:59:35","No","No","No","Internal"]
[null,null,null,13631,null,"24_01/09/2020 12:14:06 PM","2020-08-19T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Few mooring winches greasing pipes leading to roller bearings are holed.","Deck - Mooring Machinery","Mooring","Equipment Related","9.14","Medium","","","Holed pipe section to be removed and grease nipples shifted. - dual job existing and in progress.","2020-09-21T23:59:35","","Completed","2020-09-06T23:59:35","No","No","No","Internal"]
[null,null,null,13632,null,"24_01/09/2020 11:16:11 AM","2020-08-20T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Port side lifeboat fwd hatch hinge found detached.","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.29","High","","","Hinge repaired, made free and fitted onto location","2020-08-24T23:59:35","","Completed","2020-08-23T23:59:35","No","No","No","Internal","Reported completed on 7th Sept vide weekly updates on Deck maintenance"]
[null,null,null,13634,null,"24_01/09/2020 10:09:46 AM","2020-08-22T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Observed air leak from No.3 Solenoid Valve(D18) for AUS","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.8","Medium","","","valve renewed","2020-08-29T23:59:35","","Completed","2020-08-29T23:59:35","No","No","No","Internal"]
[null,null,null,13635,null,"24_01/09/2020 1:23:17 PM","2020-08-22T23:59:35","Defect","Ship Staff","Ship Staff Insp.","DURING ROUTINE INSPECTION OF MAGNETIC COMPASS ,IT IS FOUND THAT THE MAGNETIC COMPASS BASE SECURING STUDS ARE NOT TIGHT IT IS EASILY COMING OUT FROM THE HOLE.","Navigation - Others","Navigation","Equipment Related","4.9","Medium","","","Job no. DK.26 is raised in REFMAN for renewal of Magnetic Compass Base Foundation","2020-10-11T23:59:35","","Completed","2020-10-02T23:59:35","Yes","No","No","Internal"]
[null,null,null,13994,null,"24_09/09/2020 10:50:53 PM","2020-08-24T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Grease pipes on many mooring winches were found to be holed, thereby the grease is unable to reach and penetrate the winch roller bearings.","Deck - Mooring Machinery","Mooring","Equipment Related,Human Error","9.14","Medium","","","Temporary cold repairs carried out to the  holed grease pipes. Now grease is reaching all points.","2020-11-21T23:59:35","","Completed","2020-11-12T23:59:35","No","No","No","Internal"]
[null,null,null,13995,null,"24_07/09/2020 8:41:27 AM","2020-08-25T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Deck hydraulic system FWD & Aft - Vunerable pipes identified requiring replacement ","Deck - Mooring Machinery","Mooring","Equipment Related","11.4","Very High","","","Shore workshop visited vessel at Singapore, took required pipes dimensions, to fabricate ashore and supply to vessel for replacement.- Received and checked - pipes not matching with specs - flanges reordered and received. M9 hyd pipes penetration temporary repairs done. Permannent repairs to be done in DD","2021-01-21T23:59:35","","Completed","2020-12-14T23:59:35","Yes","No","No","Internal"]
[null,null,null,14000,null,"24_09/09/2020 10:57:57 PM","2020-08-25T23:59:35","Defect","Ship Staff","Suptd. Insp.","Jib head twin sheaves found completely frozen and not moving for port side hose handling crane.","Cargo Mach.","Cargo / Ballast Systems","Inappropriate Procedure","8.5","Very High","","","Sheave dismantled, area derusted and painted and sheave fitted back after lubricating and both sheaves were moving freely.","2020-09-06T23:59:35","","Completed","2020-08-27T23:59:35","No","No","No","Internal"]
[null,null,null,14001,null,"24_09/09/2020 11:02:27 PM","2020-08-26T23:59:35","Defect","Ship Staff","Ship Staff Insp.","SAAB unit was frozen after receiving TGU Communication Error","Miscellaneous","Cargo / Ballast Systems","Equipment Related","8.12","Medium","","","SAAB Technician attended vessel, renewed SCU unit and system made operational.","2020-10-01T23:59:35","","Completed","2020-09-04T23:59:35","No","No","No","Internal"]
[null,null,null,13996,null,"24_07/09/2020 8:51:21 AM","2020-08-28T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Ballast pump no.1 upper bearing overheating during test run","Deck - Machinery","Cargo / Ballast Systems","Equipment Related","8.8","Medium","","","Pump upper bearing renewed but problem persists. Bearing casing requires renewal. casing ordered. Temp to be monitored during each operation -  casing renewed on 10.12.2020. tested pump max bearing temp reached 66 deg C","2020-12-21T23:59:35","DBAU200179","Completed","2020-12-02T23:59:35","Yes","No","No","Internal"]
[null,null,null,13997,null,"24_07/09/2020 8:54:58 AM","2020-08-28T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Ballast pump no.2 upper bearing overheating during test run","Deck - Machinery","Cargo / Ballast Systems","Equipment Related","8.8","Medium","","","Bearing greasing done, old grease flushed out. tested found satisfactory. pump overhaul job added in DD refman as shaft alignment is neccesary. ","2020-12-21T23:59:35","DBAU200179","Completed","2020-12-02T23:59:35","Yes","No","No","Internal"]
[null,null,null,13998,null,"24_16/09/2020 8:45:01 PM","2020-08-29T23:59:35","Defect","Ship Staff","Ship Staff Insp.","The grease pipes on port side hose handling is unable to penertate upto the shaft due to broken grease pipe","Cargo Mach.","Crew Management","Equipment Related,Inappropriate Procedure","8.5","Very High","","","Grease pipe temporary repairs carried out and job added to REFMAN for carrying out permanent repairs in drydock.","2021-01-21T23:59:35","","Completed","2020-12-22T23:59:35","Yes","No","No","Internal"]
[null,null,null,13621,null,"24_25/08/2020 2:38:36 PM","2020-09-02T23:59:35","Defect","Ship Staff","Ship Staff Insp.","OBSERVED STBD SPRINKLER DID NOT WORK WHEN STBD L/BOAT WAS LOWERED IN WATER AT MALACCA ANCHORAGE","LSA / FFA","Safety / LSA / FFA","Inappropriate Procedure","5.29","High","","","THE L/BOAT LOWERED AGAIN IN WATER, RE-CHECKED SPRINKLERS WORKING. SYSTEM TO BE CHECKED DURING LIFEBOAT MAINTENANCE IN DD. JOB ADDED TO REFMAN","2020-12-02T23:59:35","","Completed","2020-11-24T23:59:35","Yes","No","No","Internal"]
[null,null,null,14002,null,"24_16/09/2020 8:53:12 PM","2020-09-02T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Fwd draft gauge manual hydraulic valve oil level empty","Hull & Tanks","Structural Condn. / WT integrity ","Inappropriate Procedure","11.3","Medium","","","Oil replenished and valve operation verified.","2020-09-21T23:59:35","","Completed","2020-09-03T23:59:35","No","No","No","Internal"]
[null,null,null,14083,null,"24_17/09/2020 11:39:11 PM","2020-09-05T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","VDR external unit on monkey bridge power cable leading to bridge room was sighted not water tight and sealed. A plastic sheet was wrapped to protect from rain water","Navigation - VDR / BNWAS","Navigation","Inappropriate Procedure","11.4","Very High","","","The cable penetration seale and made watertight.","2020-09-12T23:59:35","","Completed","2020-09-12T23:59:35","No","No","No","Internal"]
[null,null,null,14084,null,"24_17/09/2020 11:49:00 PM","2020-09-05T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Port life boat is not resting on the aft fender in a stowed position","LSA / FFA","Safety / LSA / FFA","Inappropriate Procedure","5.28","Very High","","","The aft fender adjusted to let the lifeboat rest completely.","2020-09-21T23:59:35","","Completed","2020-09-14T23:59:35","No","No","No","Internal"]
[null,null,null,14085,null,"24_25/09/2020 8:46:01 AM","2020-09-05T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","No.1 AC compressor unit control oil gauge defective ","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Gauge glass not clear due to glycerine - same refreshed and now readable","2020-09-05T23:59:35","","Completed","2020-09-05T23:59:35","No","No","No","Internal"]
[null,null,null,14086,null,"24_25/09/2020 8:51:42 AM","2020-09-05T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","No.2 LO purifier was in operation, noticed LO inlet temp to purifier 72 deg C","E/R - Purifier","Eng. / Strg. Comp.","Human Error","10.32","Very High","","","To maintain recommended temp of min 90 deg c at purifier inlet - - All engrs advised and temp adjusted to 90 Deg C","2020-09-05T23:59:35","","Completed","2020-09-05T23:59:35","No","No","No","Internal"]
[null,null,null,14087,null,"24_25/09/2020 8:58:29 AM","2020-09-05T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","No.1 HFO purifier was in operation and noticed HFO inlet temp at 90 deg C","E/R - Purifier","Eng. / Strg. Comp.","Human Error","10.32","Very High","","","To maintain recommended temp of min 98 deg C at purifier inlet - All engrs advised and temp adjusted to 98 Deg C","2020-09-05T23:59:35","","Completed","2020-09-05T23:59:35","No","No","No","Internal"]
[null,null,null,14088,null,"24_26/09/2020 10:37:27 AM","2020-09-05T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Emerg Mvg drill dates","E/R - Main Engine","Eng. / Strg. Comp.","Human Error","10.16","Very High","","","Dates to be displayed near the console – for third party Inspections","2020-09-05T23:59:35","","Completed","2020-09-05T23:59:35","No","No","No","Internal"]
[null,null,null,14089,null,"24_26/09/2020 10:48:35 AM","2020-09-05T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","#3 and #4 unit stuffing box drain reported higher","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","To ensure th stuffing box is fully overhauled, while carrying out liner renewal job - stuffing box for unit 3 & 4 overhauled","2020-10-05T23:59:35","","Completed","2020-09-14T23:59:35","No","No","No","Internal"]
[null,null,null,14090,null,"24_18/09/2020 10:38:50 PM","2020-09-05T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Port and stbd life boat davit limit switch is jammed, roller does not move.","LSA / FFA","Safety / LSA / FFA","Equipment Related,Inappropriate Procedure","5.28","Very High","","","Limit switch rollers were freed up after removal of paint.","2020-09-26T23:59:35","","Completed","2020-09-20T23:59:35","No","No","No","Internal"]
[null,null,null,14091,null,"24_30/09/2020 8:33:44 PM","2020-09-05T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Side rollers are completely ceased in both side Gang way ladders. ","Miscellaneous","General Appearance","Inappropriate Procedure","5.47","Medium","","","Both accommodation ladder side roller were eased up and are now rotating freely.","2020-10-03T23:59:35","","Completed","2020-09-21T23:59:35","No","No","No","Internal"]
[null,null,null,14094,null,"24_26/09/2020 10:32:41 AM","2020-09-05T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Oil max centrifugal filter LO pump was not in operation for all 3 AEs","E/R - Aux. Engine","Eng. / Strg. Comp.","Human Error","10.32","Very High","","","We had clearly advised that this pump/filter to be continuously operation – in both Engine stopped and running condition - pumps were temporarily stopped for cleaning trays for SIRE inspection - same were started afterwards.","2020-09-05T23:59:35","","Completed","2020-09-05T23:59:35","No","No","No","Internal"]
[null,null,null,14100,null,"24_26/09/2020 11:10:47 AM","2020-09-05T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","PMS - Few Jobs have not updated spares consumption properly – either there were double entried or there were no consumptions reported","Documentation","Cert. & Docu.","Human Error","10.12","Very High","","","To ensure, Stocks are updated whenever consumed - all engineers advised to follow deligently including for unplanned jobs and overhaul of standby equipment.","2020-09-05T23:59:35","","Completed","2020-09-05T23:59:35","No","No","No","Internal"]
[null,null,null,14047,null,"24_17/09/2020 11:32:03 PM","2020-09-05T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Radar performance was measured and recorded only attenuation power instead of TX/Rx transmission level","Navigation - RADAR","Navigation","Inappropriate Procedure","4.2","Medium","","","Radar performance now measured & recorded in both Tx/Rx values & attenuation values","2020-09-26T23:59:35","","Completed","2020-09-22T23:59:35","No","No","No","Internal"]
[null,null,null,14048,null,"24_18/09/2020 10:37:00 PM","2020-09-05T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Port and stbd lifeboat painter lines are wasted. Rope threads are peeling off.","LSA / FFA","Safety / LSA / FFA","External Factors","5.28","Very High","","","New painter lines made for both lifeboats","2020-10-12T23:59:35","","Completed","2020-10-21T23:59:35","No","No","No","Internal"]
[null,null,null,14049,null,"24_18/09/2020 10:41:14 PM","2020-09-05T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Em. Generator exhaust vent mesh (stbd) support was sighted with thick rust and partially damaged.","E/R - Aux. Engine","Emgcy. Systems","Inappropriate Procedure","10.32","Very High","","","Mesh supports frames to be fabricated and renewed- frames renewed","2020-10-12T23:59:35","","Completed","2020-10-12T23:59:35","No","No","No","Internal"]
[null,null,null,14050,null,"24_18/09/2020 10:43:15 PM","2020-09-05T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Provision crane stbd block swivel was found ceased.","Deck - Machinery","General Appearance","Inappropriate Procedure","8.5","Very High","","","Crane hook swivel freed up.","2020-10-16T23:59:35","","Completed","2020-10-06T23:59:35","No","No","No","Internal"]
[null,null,null,14051,null,"24_18/09/2020 10:44:51 PM","2020-09-05T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Em. generator exhaust pipe(black color) was sighted with thick rust ","E/R - Aux. Mach.","Emgcy. Systems","Inappropriate Procedure","10.32","Very High","","","Exhaust pipe derusted and painted with high temperature paint.","2020-11-07T23:59:35","","Completed","2020-11-07T23:59:35","No","No","No","Internal"]
[null,null,null,14052,null,"24_18/09/2020 10:47:48 PM","2020-09-05T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Midship draft gauge valve on stbd side was sighted sweating oil, base is corroded and wasted.","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","Inappropriate Procedure","11.2","Medium","","","Base section cold repairs carried out. Permanent repairs/renewal to be carried out in drydock. Job added to REFMAN","2020-11-10T23:59:35","","Completed","2020-11-05T23:59:35","Yes","No","No","Internal"]
[null,null,null,14053,null,"24_18/09/2020 10:52:07 PM","2020-09-05T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Both provision crane protection Guard at control box to protect accidental burst of high pressure hydraulic hose was missing.","Deck - Machinery","General Appearance","Behaviour Based,Inappropriate Procedure","8.5","Very High","","","New protecting guard covers fabricated and fitted at the control stations of both provision cranes","2020-10-21T23:59:35","","Completed","2020-10-21T23:59:35","No","No","No","Internal"]
[null,null,null,14092,null,"24_30/09/2020 9:25:34 PM","2020-09-07T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Two nos scupper plugs rubber found damaged on poop deck","Deck - Pipe / Fittings","MARPOL Related","External Factors,Inappropriate Procedure","6.2","High","","","Damaged scupper plugs were replaced with new ones","2020-09-12T23:59:35","","Completed","2020-09-08T23:59:35","No","No","No","Internal"]
[null,null,null,14093,null,"24_30/09/2020 9:31:56 PM","2020-09-07T23:59:35","Observation","Ship Staff","Ship Staff Insp.","No.1 ballast pump strainer drain valve not holding","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.44","High","","","Drain valve replaced with onboard spare","2020-09-21T23:59:35","","Completed","2020-09-12T23:59:35","No","No","No","Internal"]
[null,null,null,14055,null,"24_30/09/2020 8:45:54 PM","2020-09-07T23:59:35","Defect","Ship Staff","Ship Staff Insp.","WBT tank domes packing outer lip edges wasted for 4P, 5P, 2P, 2S, 3S, 5S","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related,Inappropriate Procedure","8.21","High","","","Job no. DK.22 raised in REFMAN for renewal of tank dome retainer channel","2020-10-19T23:59:35","","Completed","2020-10-03T23:59:35","Yes","No","No","Internal"]
[null,null,null,14056,null,"24_30/09/2020 10:39:31 AM","2020-09-09T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Ship Staff Insp.","Noted Loss of freon from Refridgeration plant no.1 ","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Plant no.2 put in use and no.1 isolated for investigation. Shaft seal renewed. tested for leaks found satisfactory.","2020-11-06T23:59:35","","Completed","2020-11-02T23:59:35","No","No","No","Internal"]
[null,null,null,14095,null,"24_30/09/2020 10:43:03 AM","2020-09-10T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Main FO supply pump no.2 leak from mech seal observed","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Pump stopped, opened and overhauled with new seal and bearings. Motor also overhauled.","2020-09-11T23:59:35","","Completed","2020-09-11T23:59:35","No","No","No","Internal"]
[null,null,null,14057,null,"24_21/09/2020 6:43:08 AM","2020-09-11T23:59:35","Observation","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","There was no objective evidence on board that the AUS, ODME\n\nsampling, cargo & water ballast pumps bulkhead seals were subjected to maintenance as per\n\nmanufacturer's manual. \n\n","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.45","High","","","Attending Supdt informed. CRF sent to include/add missing jobs in PMS. PMS updated","2020-10-04T23:59:35","","Completed","2020-10-04T23:59:35","No","No","No","External"]
[null,null,null,14058,null,"24_21/09/2020 6:47:40 AM","2020-09-11T23:59:35","Observation","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","Port & starboard aft draft marks were covered with rust/rust weeping and were illegible. ","Hull & Tanks","General Appearance","External Factors","11.2","Medium","","","Job added to REFMAN","2021-03-06T23:59:35","","Completed","2020-11-05T23:59:35","Yes","No","No","External"]
[null,null,null,14059,null,"24_30/09/2020 10:59:13 AM","2020-09-12T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Bus tie breaker MSSB to ESBD found not closing with manual push button","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","To remove from cradle and overhaul, to plan service in DD","2021-01-06T23:59:35","","Completed","2020-12-22T23:59:35","Yes","No","No","Internal"]
[null,null,null,14080,null,"24_30/09/2020 8:22:07 PM","2020-09-13T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","#4 B hyd remote valve box on deck, oil stains found inside the box","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.11","Medium","","","Self seal coupling for valve BA411 found cracked and same was replaced.","2020-09-28T23:59:35","","Completed","2020-09-22T23:59:35","No","No","No","Internal"]
[null,null,null,14082,null,"24_30/09/2020 6:09:33 PM","2020-09-13T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Windlass Hyd pipe connections/joints exposed – leading to rust/wastage","Deck - Mooring Machinery","Mooring","Equipment Related,Inappropriate Procedure","9.2","Very High","","","Pipe connections derusted, primered and covered by denso tape.Target date revised due to job prioritization.","2020-10-25T23:59:35","","Completed","2020-10-17T23:59:35","No","No","No","Internal"]
[null,null,null,14096,null,"24_26/09/2020 9:36:43 AM","2020-09-13T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Stbd Aux boiler -boiler water circulating valve (outlet from water drum) – valve bonnet nut, few of them are short and nuts not fully closed in exposing threads of nut.","E/R - Boiler","Eng. / Strg. Comp.","Human Error","10.32","Very High","","","Not a safe indication, valve bonnet holding nut should be fully closed/tightend in, exposing few threads of studs – replaced with longer studs and tightened ","2020-09-23T23:59:35","","Completed","2020-09-20T23:59:35","No","No","No","Internal"]
[null,null,null,14097,null,"24_26/09/2020 9:40:39 AM","2020-09-13T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Main engine - Fuel linkages dry and lacks greasing","E/R - Main Engine","Eng. / Strg. Comp.","Human Error","10.32","Very High","","","cleaned off old grease, greased all pivots, linkages and ensured the grease reached the right point.","2020-09-23T23:59:35","","Completed","2020-09-21T23:59:35","No","No","No","Internal"]
[null,null,null,14098,null,"24_26/09/2020 10:53:30 AM","2020-09-13T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","IG deck seal pump\t- Leaks noticed from sea water inlet valve flange bolts","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","To rectify/renew bolts - Leaky suction pipe removed and repaired, gaskets / bolts changed. ","2020-10-13T23:59:35","","Completed","2020-09-20T23:59:35","No","No","No","Internal"]
[null,null,null,14099,null,"24_26/09/2020 10:55:28 AM","2020-09-13T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Stbd side boiler inner side gauge glass seems to be not in use (isolated?)","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","To rectify and put into use -  Gauge glass was left shut after last blow down. both gauge galsses blown down and confirmed in working condition.","2020-09-28T23:59:35","","Completed","2020-09-20T23:59:35","No","No","No","Internal"]
[null,null,null,14101,null,"24_26/09/2020 10:57:21 AM","2020-09-13T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Port side gaige glass diff in water level between inner and outr units  - WL should be at same height","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","To check if any valves are partially shut and rectify - The water level was below normal level and hence was not showing in upper gauge, both gauge glasses blown down and confirmed in working condition","2020-09-28T23:59:35","","Completed","2020-09-20T23:59:35","No","No","No","Internal"]
[null,null,null,14102,null,"24_30/09/2020 8:11:26 PM","2020-09-13T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","2C PV valve noticed leaking from pressure side ","Cargo Mach.","Cargo / Ballast Systems","Equipment Related,Inappropriate Procedure","8.21","High","","","Spare PV valve overhauled and leaking PV valve replaced.","2020-10-03T23:59:35","","Completed","2020-09-20T23:59:35","No","No","No","Internal"]
[null,null,null,14054,null,"24_26/09/2020 11:31:34 AM","2020-09-13T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Engine room Sky light - Lips corroded","Miscellaneous","General Appearance","External Factors","11.8","Low","","","Job no. DK.30 has been added to REFMAN for Engine Room Maintenance Hatch Repair","2020-10-13T23:59:35","","Completed","2020-09-30T23:59:35","Yes","No","No","Internal"]
[null,null,null,14060,null,"24_26/09/2020 9:44:54 AM","2020-09-13T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Cylinder head all drains/hidden locationsdirty","E/R - Main Engine","Eng. / Strg. Comp.","Human Error","10.32","Very High","","","To clean/soap wash and ensure all surrounding areas of cyl head are maintained clean to easily identify leaks if any - all areas around cyl heads, jackets, fuel pumps and below cleaned up and painted.","2020-10-08T23:59:35","","Completed","2020-10-04T23:59:35","No","No","No","Internal"]
[null,null,null,14061,null,"24_26/09/2020 9:57:15 AM","2020-09-13T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","HFO purifier no.1 - Vibration observed whilst in operation","E/R - Purifier","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","To stop, check, if any trouble with bowl/bearings- Purifier was stopped on 14th Feb 2020 and standby purifier put in use. Target date extended due to other job prioritization. Purifier opened up for inspection and cleaning of bowl - found uneven sludge deposits - completed cleaning. tested and found satisfactory.","2020-10-13T23:59:35","","Completed","2020-10-12T23:59:35","No","No","No","Internal"]
[null,null,null,14062,null,"24_26/09/2020 10:00:27 AM","2020-09-13T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Tube light fitting acrylic covers - Few very dirty and dull","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Human Error","10.32","Very High","","","To soap wash and if faded , order for new acrylic covers - cleaned all, replacement not requried.","2020-10-03T23:59:35","","Completed","2020-09-28T23:59:35","No","No","No","Internal"]
[null,null,null,14063,null,"24_26/09/2020 10:51:18 AM","2020-09-13T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","All 3 AEs exhaust uptakes, drain seal pots were empty – also no gas passing was observed","E/R - Aux. Engine","Eng. / Strg. Comp.","Human Error","10.32","Very High","","","To check if drain lines are clear and ensure seal pot is always filled and kept -  Checked pipes and cleared, water filled for AE no.1, 2 &3.","2020-09-28T23:59:35","","Completed","2020-09-22T23:59:35","No","No","No","Internal"]
[null,null,null,14064,null,"24_26/09/2020 11:00:04 AM","2020-09-13T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Incinerator - Exhaust drain seal pot empty","E/R - Aux. Mach.","Eng. / Strg. Comp.","Human Error","10.32","Very High","","","To ensure the drain line is clear and the seal water is always maintained - confirmed clear and water filled","2020-09-20T23:59:35","","Completed","2020-09-14T23:59:35","No","No","No","Internal"]
[null,null,null,14065,null,"24_26/09/2020 11:03:34 AM","2020-09-13T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Spares Inventory - Still pending to be completed for all equipment ","Miscellaneous","Eng. / Strg. Comp.","Human Error","10.12","Very High","","","Checks and updation started in Feb with target dates of end July – still pending -  to be checked and updated - target date revised as found that all spares parts need to be rechecked, also not able to complete due to other jobs prioritization - all spares checked and updated in PAL ","2020-12-12T23:59:35","","Completed","2020-12-06T23:59:35","No","No","No","Internal"]
[null,null,null,14066,null,"24_26/09/2020 11:18:06 AM","2020-09-13T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Funnel - Uptakes/Goose neck dirty","Miscellaneous","General Appearance","Equipment Related","11.8","Low","","","Funnel exhaust stack derusted/cleaned and applied with HT paint. Target date revised due to job prioritization and awaiting clear weather day","2020-10-23T23:59:35","","Completed","2020-10-21T23:59:35","No","No","No","Internal"]
[null,null,null,14067,null,"24_26/09/2020 11:24:57 AM","2020-09-13T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Receptacle junction boxes - Various receptacle junction boxes on poop deck/china passage holding brackets are corroded/wasted","Deck - Pipe / Fittings","General Appearance","External Factors","11.8","Low","","","To check if new support brackets can be welded or drill and secure wih a ew frame. -Target date extended as per job prioritization.  two boxes for cranes power switch fabricated - fixed by nut bolts.","2020-10-16T23:59:35","","Completed","2020-10-15T23:59:35","No","No","No","Internal"]
[null,null,null,14068,null,"24_26/09/2020 11:28:46 AM","2020-09-13T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Tube light cable penteration\tOne tube light cable penetration on port side engine casing (china passage) corroded/wasted","Elect. Mach. & Equip.","General Appearance","External Factors","11.8","Low","","","To check and look at possibility of cut/renew the section - Target date extended due to job prioritization & planning. Penetration pipe renewed by hot work ","2020-12-12T23:59:35","","Completed","2020-12-08T23:59:35","No","No","No","Internal","Basis job being planned shortly, target date extended till end Nov"]
[null,null,null,14069,null,"24_26/09/2020 11:34:51 AM","2020-09-13T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Bunker tanks - Bunker tanks vent pipes collecting tray coaming lips at various stages of corossion","Deck - Pipe / Fittings","General Appearance","External Factors","11.7","High","","","Job Dk 62 added to REFMAN for carrying out repairs during dry dock.","2020-11-13T23:59:35","","Completed","2020-11-02T23:59:35","Yes","No","No","Internal"]
[null,null,null,14070,null,"24_26/09/2020 11:38:08 AM","2020-09-13T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Sunken deck access  - Ladder stair case supports below on deck on to the bulkhed is corroded and wasted","Deck - Pipe / Fittings","General Appearance","External Factors","11.7","High","","","Job No. Dk 31 included for crop & renewal of inclined ladder lugs","2020-10-13T23:59:35","","Completed","2020-10-03T23:59:35","Yes","No","No","Internal"]
[null,null,null,14071,null,"24_30/09/2020 5:03:46 PM","2020-09-13T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Stbd side accomm front fire hose box hinges damaged","LSA / FFA","Safety / LSA / FFA","Equipment Related,Inappropriate Procedure","5.35","Medium","","","Box hinge renewed and door repaired","2020-10-03T23:59:35","","Completed","2020-09-27T23:59:35","No","No","No","Internal"]
[null,null,null,14072,null,"24_30/09/2020 5:06:01 PM","2020-09-13T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Both side davit’s brake releasing lever thinned down","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.28","Very High","","","Brake release lever wasted section cropped & renewed.","2020-10-03T23:59:35","","Completed","2020-09-30T23:59:35","No","No","No","Internal"]
[null,null,null,14073,null,"24_30/09/2020 5:09:18 PM","2020-09-13T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Both side gangway motors exterior dirty/rusty","Deck - Machinery","General Appearance","Equipment Related","5.47","Medium","","","Both accommodation ladder motors derusted and painted.Target date revised as job prioritized and planned to be carried out on rainy day.","2020-10-08T23:59:35","","Completed","2020-10-18T23:59:35","No","No","No","Internal"]
[null,null,null,14074,null,"24_30/09/2020 5:13:41 PM","2020-09-13T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Both gangway landing platforms thinned down.","Deck - Pipe / Fittings","General Appearance","Equipment Related","5.47","Medium","","","Job DK 32 has been added to REFMAN for carrying out permanent repairs in drydock.","2020-10-13T23:59:35","","Completed","2020-10-05T23:59:35","Yes","No","No","Internal"]
[null,null,null,14075,null,"24_30/09/2020 5:21:19 PM","2020-09-13T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Billy Pugh basket delivered in 2015","Miscellaneous","General Appearance","Equipment Related","5.47","Medium","","","Inspection of Personnel Basket carried out as per maker and found to be in good condition","2020-09-28T23:59:35","","Completed","2020-09-28T23:59:35","No","No","No","Internal","Shall be sending new revised guidelines for renewal of the PTB every 4 years, hence amended target date to end Dec"]
[null,null,null,14076,null,"24_30/09/2020 5:26:38 PM","2020-09-13T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Main deck stay wires – look rusty and devoid of grease","Miscellaneous","General Appearance","External Factors","11.3","Medium","","","Stay wires greasing carried out","2020-10-08T23:59:35","","Completed","2020-10-06T23:59:35","No","No","No","Internal"]
[null,null,null,14077,null,"24_30/09/2020 5:30:01 PM","2020-09-13T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Most of the foam monitor turret springs are rusted","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.38","High","","","All foam monitor turret springs inspected, 3 nos foam monitor springs renewed with onboard spares.","2020-10-03T23:59:35","","Completed","2020-09-28T23:59:35","No","No","No","Internal"]
[null,null,null,14078,null,"24_30/09/2020 7:55:15 PM","2020-09-13T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Manifold, walkways lot of metallic gratings were found wasted/ corroded","Deck - Pipe / Fittings","General Appearance","Equipment Related,Inappropriate Procedure","6.6","Medium","","","Gratings renewal completed","2020-11-13T23:59:35","DBAU200222","Completed","2020-11-08T23:59:35","No","No","No","Internal","As required items were already supplied recently - Pls close once the existing supplied items are consumed and create new job with new target dates.\n\nHence had amended target date to end Nov"]
[null,null,null,14079,null,"24_30/09/2020 8:20:41 PM","2020-09-13T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Few foam monitors found leaking","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.38","High","","","Leaks rectified by overhauling","2020-10-13T23:59:35","","Completed","2020-10-11T23:59:35","No","No","No","Internal","Raise RO if reqd for the job and then set target date, else this job should be taken on priority and complete."]
[null,null,null,14103,null,"24_30/09/2020 9:46:48 PM","2020-09-14T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Both port and stbd lifeboat gripe trigger hooks movement not free.","LSA / FFA","Safety / LSA / FFA","Equipment Related,Inappropriate Procedure","5.28","Very High","","","Both lifeboat gripe trigger hooks dismantled and freed up after derusting.","2020-09-21T23:59:35","","Completed","2020-09-20T23:59:35","No","No","No","Internal"]
[null,null,null,14104,null,"24_30/09/2020 10:47:36 AM","2020-09-18T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Noted during inspection Aft hyd station pumps/motors coupling spider in deteriorated condition","Deck - Mooring Machinery","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Renewed coupling spider for all four pumps/motors.","2020-09-19T23:59:35","","Completed","2020-09-19T23:59:35","No","No","No","Internal"]
[null,null,null,14263,null,"24_15/10/2020 10:00:11 PM","2020-09-24T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Pumproom winch air motor not working","Deck - Machinery","Cargo / Ballast Systems","Equipment Related,External Factors","5.2","Very High","","","Pumproom air motor overhauling carried out and made opearational","2020-10-06T23:59:35","","Completed","2020-09-26T23:59:35","No","No","No","Internal"]
[null,null,null,14264,null,"24_15/10/2020 10:05:56 PM","2020-09-24T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Forward fire line pressure gauge defective","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.35","Medium","","","New pressure gauge fitted to replace defective one.","2020-10-06T23:59:35","","Completed","2020-09-27T23:59:35","No","No","No","Internal"]
[null,null,null,14265,null,"24_16/10/2020 6:44:37 AM","2020-09-24T23:59:35","Defect,Observation","Ship Staff","Ship Staff Insp.","AE 1 & 2 noted JCW and LO temps not maintaining correct required temperature - thermostatic elements suspected not working properly","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","AE 1 & 2 JCW & LO thermostatic elemnts inspected, checked opening temps using calibrator. defective ones renewed together with the o-rings. Tested engines and noted significant change in temps and maintaining as required.","2020-10-09T23:59:35","","Completed","2020-10-04T23:59:35","No","No","No","Internal"]
[null,null,null,13440,null,"24_15/08/2020 9:08:19 PM","2020-09-27T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Port side accommodation ladder shifting guide rail trackway platform found cracked and bend.","Miscellaneous","General Appearance","External Factors","5.47","Medium","","","Repairs to be carried out. Awaiting opportunity as repairs will require hotwork, tank preparation. Temporary support plate fixed after straightening the bent plate. Job added to Refman list for permanent repairs in DD","2020-12-28T23:59:35","","Completed","2020-12-27T23:59:35","Yes","No","No","Internal"]
[null,null,null,14258,null,"24_16/10/2020 6:17:37 AM","2020-09-27T23:59:35","Defect,Observation","Ship Staff","Ship Staff Insp.","All Aux engines resilient mountings height found below maker's recommendation.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","To renew resilient mountings for all Aux Engines. RO raised for new mountings. DBAU205076 RECEIVED one set - Replaced on AE no.3 on 24th Nov. Awaiting spares supply for other two AEs. Defect transferred to Refman list for DD.","2020-12-28T23:59:35","DBAU200193","Completed","2020-12-27T23:59:35","Yes","No","No","Internal"]
[null,null,null,14266,null,"24_16/10/2020 6:26:40 AM","2020-09-27T23:59:35","Defect,Observation","Ship Staff","Ship Staff Insp.","During quarterly test of emergency stops noted ES1 & ES2 on ESBD not working - no.2 Main FO supply & circ pumps, ER vent fan no.2 not tripped","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","The defective ‘Line Fault Detector’ replaced with new one in ESBD; same working satisfactorily","2020-10-04T23:59:35","","Completed","2020-10-03T23:59:35","No","No","No","Internal"]
[null,null,null,14267,null,"24_16/10/2020 6:36:39 AM","2020-09-27T23:59:35","Defect,Observation","Ship Staff","Ship Staff Insp.","AE no.2 - no.5 unit cyl head jacket seemed loose during operation - noted slight movement.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Cyl head removed and jacket secured properly, bolt found loose. assembled and tested, found satisfactory","2020-10-01T23:59:35","","Completed","2020-10-01T23:59:35","No","No","No","Internal"]
[null,null,null,14259,null,"24_16/10/2020 6:08:44 AM","2020-09-29T23:59:35","Defect,Observation","Ship Staff","Ship Staff Insp.","Slight oil leak observed from the balance valve connection to luffing cylinder body of Hose handling crane (S)","Deck - Machinery","General Appearance","Equipment Related","8.5","Very High","","","Valve removed, body chipped cleaned and fixed back with new O-ring. Tested crane luffing observed no leaks. The valve body is corroded heavily. RO DBAU200230 raised for new valve. Crane health check job added in Refman. valve to be replaced once recieved.","2020-12-30T23:59:35","DBAU200230","Completed","2020-12-29T23:59:35","Yes","No","No","Internal"]
[null,null,null,14268,null,"24_16/10/2020 6:31:14 AM","2020-09-30T23:59:35","Defect,Observation","Ship Staff","Ship Staff Insp.","Emergency air bottle drain line pot top flange made of perpex glass - can shatter under pressure and cause injury","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Flange replaced with metal one with holes to avoid pressure build-up.","2020-09-30T23:59:35","","Completed","2020-09-30T23:59:35","No","No","No","Internal"]
[null,null,null,14269,null,"24_15/10/2020 11:56:03 PM","2020-10-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Port and stbd side aft bunker station drip trays base is not welded onto main deck and tray is presently secured with nut/bolts arrangement.","Deck - Pipe / Fittings,Hull & Tanks","Structural Condn. / WT integrity ","Equipment Related,Inappropriate Procedure","6.6","Medium","","","Job DK 35 added to REFMAN for tray base to be permanently welded onto main deck.","2020-10-16T23:59:35","","Completed","2020-10-05T23:59:35","Yes","No","No","Internal"]
[null,null,null,14261,null,"24_16/10/2020 12:04:14 AM","2020-10-03T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Mooring winch brake cylinder seal leaking for winch M1A.","Deck - Mooring Machinery","Mooring","Equipment Related","9.14","Medium","","","Mooring winch brake cylinder replaced with onboard spare.","2020-10-10T23:59:35","","Completed","2020-10-07T23:59:35","No","No","No","Internal"]
[null,null,null,14262,null,"24_16/10/2020 12:08:58 AM","2020-10-03T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Mooring winch brake cylinder for winch M6B, found having heavy corrosion.","Deck - Mooring Machinery","Mooring","Equipment Related,External Factors","9.14","Medium","","","Brake cylinder derusted and painted.","2020-10-17T23:59:35","","Completed","2020-10-08T23:59:35","No","No","No","Internal"]
[null,null,null,13618,null,"24_28/08/2020 11:57:50 AM","2020-10-09T23:59:35","Defect,Observation","Ship Staff","Ship Staff Insp.","Port Provision crane general condition not satisfactory - Hyd luffing circuit balance valve, some connections in wasted condition, operator's platform railings wasted, control block cover wasted.","Deck - Machinery","General Appearance","Equipment Related","8.5","Very High","","","Operator platform railings renewed, control block cover repair completed, luffing circuit balance valve and limit valve RO raised. Job added to Refman list for crane heallth check and repaires in DD","2021-01-09T23:59:35","DBAU200198, DBAU210067","Completed","2021-01-11T23:59:35","Yes","No","No","Internal"]
[null,null,null,14391,null,"24_31/10/2020 9:09:45 AM","2020-10-11T23:59:35","Defect","Ship Staff","Ship Staff Insp.","AE DO pumps 1 & 2 both coupling spiders found in damaged condition during inspection","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","both coupling spiders renewed with spare new","2020-10-11T23:59:35","","Completed","2020-10-11T23:59:35","No","No","No","Internal"]
[null,null,null,14392,null,"24_31/10/2020 9:13:13 AM","2020-10-11T23:59:35","Defect","Ship Staff","Ship Staff Insp.","EGE feed water pump no.2 coupling bolt rubbers were noted in damaged condition","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related,Human Error","10.32","Very High","","","Coupling bolt rubbers renewed with spare new set","2020-10-11T23:59:35","","Completed","2020-10-11T23:59:35","No","No","No","Internal"]
[null,null,null,14389,null,"24_31/10/2020 9:25:36 AM","2020-10-13T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Control air compressor tripping on high air temperature","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","checked thorougly and found primary reason as lower than normal oil level. higher Oil carry over can be due to separator filter, no spare onboard. Also found air/oil cooler with temporary repairs. raised RO for new cooler, separator and air filters. A new compressor received and installed.  working satisfactory","2021-01-21T23:59:35","","Completed","2021-01-07T23:59:35","No","No","No","Internal"]
[null,null,null,13999,null,"24_16/09/2020 9:05:12 PM","2020-10-16T23:59:35","Defect","Ship Staff","Ship Staff Insp.","C-deck port side accommodation entrance door not closing properly","Accommodation","General Appearance","Equipment Related","11.6","Medium","","","Door repair works to be carried out. Hotwork required in place, Job added to Refman list for attendance in DD","2021-01-16T23:59:35","","Completed","2021-01-11T23:59:35","Yes","No","No","Internal"]
[null,null,null,14390,null,"24_30/10/2020 10:50:45 PM","2020-10-17T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Stbd side manifold pressure & temperature gauge box broken","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related,External Factors","8.13","Medium","","","Pressure/temperature gauge box repaired and fixed back on stbd manifold.","2020-11-11T23:59:35","","Completed","2020-11-01T23:59:35","No","No","No","Internal"]
[null,null,null,13623,null,"24_26/08/2020 7:12:39 AM","2020-10-17T23:59:35","Defect","Ship Staff","Ship Staff Insp.","BALLAST GAS DETECTION SYSTEM GIVING FAULT ALARM.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.46","Very High","","","3 Nos 2-waysolenoid valve overhauled. 3 Nos solenoid valve repaired with used parts. Vacuum switch and pressure switch setting readjusted. All sample line filters inspected and 3 Nos filter renewed. Cleaned LEL sensor and calibrated with span gas. Flow fault, Pump failure, LEL  5% & 10% alarms are tried out. Every few days some solenoid valve gives fault and requires overhaul / attention. The system performance is being monitored. spares received and to atend again. 17.12.20 All solenoid valves overhauled, both vaccum pumps overhauled with new diaphragms and valve plates. checked system for internal leakage. cabinet cooling fan renewed. system put in use - under observation. 19.12.20: Internal leakage alarm persisted - checked and found void space valve remaining on due to PCB RIOK-41 fault. PCB ordered and to be renewed in DD. Job added in Refman list","2021-01-17T23:59:35","DBAU210012","Completed","2021-01-15T23:59:35","Yes","No","No","Internal"]
[null,null,null,14393,null,"24_30/10/2020 10:58:46 PM","2020-10-17T23:59:35","Defect,Other","Ship Staff","Ship Staff Insp.","Leak observed from hydroblaster rotating nozzle during operation.","Deck - Machinery,Miscellaneous","General Appearance","Equipment Related","11.4","Very High","","","Self rotating nozzle overhauling carried out, worn out parts replaced and nozzle leak rectified.","2020-10-27T23:59:35","","Completed","2020-10-18T23:59:35","No","No","No","Internal"]
[null,null,null,13252,null,"24_29/07/2020 2:32:58 PM","2020-10-21T23:59:35","Other","Owner / Marine / Tech. Suptd.","Nav Audit / Verification","To install CCTV in ECR,CCR and Bridge wings","Elect. Mach. & Equip.","General Appearance","Equipment Related","4.1","High","","","Raised as per office request - Received parts -Job added to Refman list for DD","2021-01-21T23:59:35","","Completed","2021-01-15T23:59:35","Yes","No","No","Internal"]
[null,null,null,13633,null,"24_31/08/2020 8:47:08 AM","2020-10-22T23:59:35","Defect","Ship Staff","Ship Staff Insp.","OBSERVED ENG ROOM MAIN STEAM VV DELIVERY TO MAIN DECK IS NOT HOLDING.STEAM PIPES ON DECK ARE REMAINING HOT CONTINUOUSLY.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.2","Low","","","Either the main steam or warming up steam valve is suspected. steam sys needs to be shut and valves inspected. RO for warming up valve raised, Job added to Refman list for overhaul of valves in DD.","2021-01-21T23:59:35","DBAU200204","Completed","2021-01-15T23:59:35","Yes","No","No","Internal"]
[null,null,null,14640,null,"24_15/11/2020 10:32:37 PM","2020-10-24T23:59:35","Defect","Ship Staff","Ship Staff Insp.","MW10 mooring winch standing platform frames and supports wasted/corroded.","Deck - Pipe / Fittings","Mooring","Equipment Related,Inappropriate Procedure","9.14","Medium","","","New standing platform fabricated and fitted","2020-11-11T23:59:35","","Completed","2020-11-14T23:59:35","No","No","No","Internal","Target date set less, hence amended to  end Nov"]
[null,null,null,14648,null,"24_10/11/2020 5:57:32 AM","2020-10-24T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Sewage discharge pump no.2 mech seal leaking slightly","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Pump dismantled and mech seal renewed. tested observed no leakage.","2020-10-25T23:59:35","","Completed","2020-10-25T23:59:35","No","No","No","Internal"]
[null,null,null,14649,null,"24_10/11/2020 6:29:47 AM","2020-10-24T23:59:35","Critical Equipment,Defect,Non Conformity","Ship Staff","Ship Staff Insp.","ME OMD sensor for chaincase noted to be defective and also not included in configuration of OMD control panel","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related,Human Error","10.32","Very High","","","Sensor renewed, OMD panel configuration changed to include this sensor. tested the sensor and observed working satisfactorily.","2020-10-24T23:59:35","","Completed","2020-10-24T23:59:35","No","No","No","Internal"]
[null,null,null,14650,null,"24_15/11/2020 10:44:12 PM","2020-10-24T23:59:35","Defect","Ship Staff","Ship Staff Insp.","No.2 ballast eductor nrv bolt corroded","Cargo Mach.","Cargo / Ballast Systems","Equipment Related,External Factors","11.4","Very High","","","New bolt fitted to the nrv","2020-11-05T23:59:35","","Completed","2020-11-01T23:59:35","No","No","No","Internal"]
[null,null,null,14651,null,"24_10/11/2020 6:36:06 AM","2020-10-25T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Noted low insulation alarm from MSBD 440 V - traced to Gally cooking range","Accommodation,Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Investigated and found temperature control switch defective for no. 1 hotplate - switch renewed","2020-10-25T23:59:35","","Completed","2020-10-25T23:59:35","No","No","No","Internal"]
[null,null,null,14652,null,"24_10/11/2020 6:02:34 AM","2020-10-26T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Incinerator flue gas fan - noted increased vibrations","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Fan inlet bellow, pipe and cover dismantled. Fan cleaned and checked. Drive shaft plummer bearings covers opened and regreasing done. assembled and tested noted improvement. Job added to Refman for fan balancing.  ","2020-10-27T23:59:35","","Completed","2020-10-27T23:59:35","Yes","No","No","Internal"]
[null,null,null,14653,null,"24_15/11/2020 10:37:37 PM","2020-10-26T23:59:35","Defect","Ship Staff","Ship Staff Insp.","1S, 3P & 5C IG branch valves found hard to operate.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related,External Factors","8.3","Very High","","","Valves overhauling carried out and valve movement made free.","2020-11-06T23:59:35","","Completed","2020-11-03T23:59:35","No","No","No","Internal"]
[null,null,null,14654,null,"24_15/11/2020 10:48:58 PM","2020-10-28T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Mooring winch M7B brake cylinder unable to develop pressure for releasing brakes","Deck - Machinery","Mooring","Equipment Related","9.14","Medium","","","Brake cylinder renewed with onboard spare","2020-11-04T23:59:35","","Completed","2020-11-04T23:59:35","No","No","No","Internal"]
[null,null,null,14655,null,"24_15/11/2020 6:15:15 AM","2020-10-29T23:59:35","Critical Equipment,Defect","Ship Staff","Ship Staff Insp.","During weekly checks on Fire detection system found Manual call point defective near elevator on ER 1st deck","LSA / FFA","Eng. / Strg. Comp.","Equipment Related","5.35","Medium","","","replaced with spare one. RO raised for new one","2020-11-01T23:59:35","DBAU200219","Completed","2020-11-01T23:59:35","No","No","No","Internal"]
[null,null,null,14656,null,"24_10/11/2020 6:40:35 AM","2020-10-29T23:59:35","Defect","Ship Staff","Ship Staff Insp.","REPEAT ENTRY","Miscellaneous","General Appearance","Equipment Related","","","","","REPEAT ENTRY","2020-11-13T23:59:35","","Completed","2020-11-01T23:59:35","No","No","No","Internal"]
[null,null,null,14657,null,"24_10/11/2020 6:07:59 AM","2020-10-30T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Aux Boiler FO pump no.1 mech seal leakage noted","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","pump overhauled with new mech seal,ball bearing,balance piston,bearing seal, thrust seal,distance piece,throat bush, oil seal,bearing nut and washer and drive shaft. Tested and observed working satisfactorily without any leakage.","2020-10-31T23:59:35","","Completed","2020-10-31T23:59:35","No","No","No","Internal"]
[null,null,null,14641,null,"24_10/11/2020 6:21:01 AM","2020-10-31T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Noted crack on the foundation frame below the AC compressor no.2","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Hot work repair is required. to plan at the time of compressor renewal, awaiting supply of same. Job added to Refman list for DD attendance","2021-01-31T23:59:35","","Completed","2021-01-15T23:59:35","Yes","No","No","Internal"]
[null,null,null,14642,null,"24_15/11/2020 10:27:22 PM","2020-11-03T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Fire hydrant on bridge deck stbd side found leaking.","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.38","High","","","Hydrant overhauled and leak rectified","2020-11-10T23:59:35","","Completed","2020-11-07T23:59:35","No","No","No","Internal","Target dat set very less, hence increased till end Nov"]
[null,null,null,14643,null,"24_15/11/2020 5:07:44 AM","2020-11-04T23:59:35","Defect","Ship Staff","Ship Staff Insp.","During 8000 hrs routine of LO purifier no.2 noted water seapage past the vertical shaft to bearings, shaft in quite corroded condition","E/R - Purifier","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","shaft and bearings renewed. assembled and tested . working satisfactorily.","2020-11-09T23:59:35","","Completed","2020-11-09T23:59:35","No","No","No","Internal"]
[null,null,null,14645,null,"24_15/11/2020 10:17:39 PM","2020-11-04T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Mast Riser Flame Screen Cover edges cracked from weld seam","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related,Inappropriate Procedure","8.4","Medium","","","Cracked areas welded after taking cover to engine room workshop","2020-11-21T23:59:35","","Completed","2020-11-21T23:59:35","No","No","No","Internal"]
[null,null,null,14646,null,"24_15/11/2020 10:21:32 PM","2020-11-04T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Mast riser vent head coaming thinned down and sump base plate holed.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related,Inappropriate Procedure","8.4","Medium","","","Jobs DK 53 has been added to REFMAN to carry out permanent sump base plate cold repairs.","2020-12-03T23:59:35","","Completed","2020-11-18T23:59:35","Yes","No","No","Internal"]
[null,null,null,14647,null,"24_15/11/2020 10:23:57 PM","2020-11-04T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Mast riser drain valve stub piece wasted/corroded.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related,Inappropriate Procedure","8.4","Medium","","","Job  DK 53 has been added to REFMAN for carrying out permanent repairs.","2020-12-03T23:59:35","","Completed","2020-11-18T23:59:35","Yes","No","No","Internal"]
[null,null,null,15422,null,"24_30/11/2020 8:49:05 PM","2020-11-07T23:59:35","Defect","Ship Staff","Ship Staff Insp.","1S COW machine valve is hard to operate","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related,External Factors","8.34","High","","","Valve overhauled and eased up","2020-11-14T23:59:35","","Completed","2020-11-09T23:59:35","No","No","No","Internal"]
[null,null,null,15423,null,"24_30/11/2020 8:56:54 PM","2020-11-07T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Foam line block valve inside foam room was found hard to operate","LSA / FFA","Safety / LSA / FFA","Equipment Related,Inappropriate Procedure","5.35","Medium","","","Valve overhauled and eased up","2020-11-11T23:59:35","","Completed","2020-11-08T23:59:35","No","No","No","Internal"]
[null,null,null,15431,null,"24_30/11/2020 9:07:49 PM","2020-11-07T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Fire hydrant on forecastle deck leaking","LSA / FFA","Safety / LSA / FFA","Equipment Related,Inappropriate Procedure","5.38","High","","","Hydrant overhauled and leak rectified","2020-11-12T23:59:35","","Completed","2020-11-09T23:59:35","No","No","No","Internal"]
[null,null,null,15424,null,"24_01/12/2020 4:29:33 AM","2020-11-10T23:59:35","Critical Equipment,Defect","Ship Staff","Ship Staff Insp.","When tested steering gear in emergency mode noted rudder found not remaining steady and slowly moving either Port or Stbd side depending upon motor in use. Also noted error in rudder angle indicator and actual position","Critical Equip.","Eng. / Strg. Comp.","Equipment Related","10.39","High","","","Adjustment made on each pump swash plate control mechanism as per the manual and became steady. Also alignment done between the rudder angle transmitter and angle indicators on the bridge and now showing same reading.","2020-11-11T23:59:35","","Completed","2020-11-10T23:59:35","No","No","No","Internal"]
[null,null,null,15425,null,"24_01/12/2020 4:42:52 AM","2020-11-12T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Noted W/H printer paper collecting unit was not working. ","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Motor and motor controls PCB were defective. Motor [5 Volt D.C] has been replaced with old C.D drive motor, modified the motor control PCB and fitted; working satisfactorily","2020-11-12T23:59:35","","Completed","2020-11-12T23:59:35","No","No","No","Internal"]
[null,null,null,15426,null,"24_30/11/2020 11:13:20 AM","2020-11-14T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Noted pressure drop accros FW Re-hardening filter affecting the FW supply to accomodation","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Inspection covers opened, Dolomite physically removed and washed outside, both inlet outlet filters renewed. Dolomite refilled and tested. working satisfactorily","2020-11-18T23:59:35","","Completed","2020-11-18T23:59:35","No","No","No","Internal"]
[null,null,null,15427,null,"24_30/11/2020 9:21:48 PM","2020-11-14T23:59:35","Defect","Ship Staff","Ship Staff Insp.","One drain pipe on poop deck aft leading from atop acetylene room choked","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.4","Very High","","","Drain pipe choke cleared","2020-11-28T23:59:35","","Completed","2020-11-16T23:59:35","No","No","No","Internal"]
[null,null,null,15428,null,"24_30/11/2020 11:22:24 AM","2020-11-17T23:59:35","Other","Ship Staff","Ship Staff Insp.","MAC no.1 LO low pressure alarm received after LO renewal","E/R - Air Comp.","Eng. / Strg. Comp.","External Factors","10.32","Very High","","","Checked and found sump oil discoloured and with fowl odour & precipitation. Suspected the oil from the new LO bucket was the reason. Oil refilled from new bucket, filter renewed and tested comp. working satisfactorily.","2020-11-19T23:59:35","","Completed","2020-11-18T23:59:35","No","No","No","Internal"]
[null,null,null,15429,null,"24_01/12/2020 4:36:05 AM","2020-11-17T23:59:35","Defect","Ship Staff","Ship Staff Insp.","During routine testing of standby starts of pumps, noted faulty electronic motor start module for LT CFW Pump no. 1 and 3 ","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Electronic motor start module for LT CFW Pump no. 1 and 3 renewed nad tested standby start. working satisfactorily","2020-11-17T23:59:35","","Completed","2020-11-17T23:59:35","No","No","No","Internal"]
[null,null,null,15420,null,"24_30/11/2020 9:10:51 PM","2020-11-21T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Foam line drain valve found leaking","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.38","High","","","Valve overhauled and leak rectified","2020-11-28T23:59:35","","Completed","2020-11-22T23:59:35","No","No","No","Internal"]
[null,null,null,15430,null,"24_30/11/2020 9:04:05 PM","2020-11-21T23:59:35","Defect","Ship Staff","Ship Staff Insp.","AUS vacuum pump no.1 source indication lamp not working","Elect. Mach. & Equip.","Cargo / Ballast Systems","Equipment Related","8.8","Medium","","","Lamp renewed","2020-11-22T23:59:35","","Completed","2020-11-22T23:59:35","No","No","No","Internal"]
[null,null,null,15746,null,"24_11/12/2020 1:22:14 PM","2020-11-22T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Stbd side no.3 cargo manifold outer drain valve CL312 observed to be hard to operate","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related,Inappropriate Procedure","8.11","Medium","","","Drain valve CL312 overhauled and valve made free.","2020-11-29T23:59:35","","Completed","2020-11-24T23:59:35","No","No","No","Internal"]
[null,null,null,15747,null,"24_15/12/2020 7:07:31 AM","2020-11-22T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Noted during last AEs performance test that the KVa load is not shared equally amongst onload AEs","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Investigated and found AE no. 1 no load voltage is less compared to others and lot less than shop trial values. AVR set voltage fine tuning done and tested parallel operation of all AEs. Noted KVa approx equal sharing and satisfactory.","2020-12-05T23:59:35","","Completed","2020-12-02T23:59:35","No","No","No","Internal"]
[null,null,null,15738,null,"24_11/12/2020 1:09:29 PM","2020-11-23T23:59:35","Defect","Ship Staff","Ship Staff Insp.","MW3B mooring winch drum end sheared from the slot provided to connect lock pin for test kit support.","Deck - Mooring Machinery","Mooring","Equipment Related","9.15","Medium","","","job added to REFMAN to carry out permanent repairs in DD","2021-02-08T23:59:35","","Completed","2021-01-11T23:59:35","Yes","No","No","Internal"]
[null,null,null,15748,null,"24_11/12/2020 1:12:33 PM","2020-11-23T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Valve wheel for fresh water line on upper deck aft broken","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.4","Very High","","","Valve wheel renewed","2020-11-30T23:59:35","","Completed","2020-11-25T23:59:35","No","No","No","Internal"]
[null,null,null,15749,null,"24_11/12/2020 1:18:08 PM","2020-11-23T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Port side A-deck outside door locking arrangement damaged and door unable to be locked.","Accommodation","General Appearance","Equipment Related","11.6","Medium","","","New locking arrangement fitted and rectified","2020-11-30T23:59:35","","Completed","2020-11-26T23:59:35","No","No","No","Internal"]
[null,null,null,15750,null,"24_11/12/2020 2:18:17 PM","2020-11-23T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Fire line drain valve was found leaking while the fire pump was in operation","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.38","High","","","Leaking drain valve renewed with new spare valve.","2020-11-30T23:59:35","","Completed","2020-11-26T23:59:35","No","No","No","Internal"]
[null,null,null,15751,null,"24_11/12/2020 2:15:14 PM","2020-11-26T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Stbd windlass fwd operating lever block in seized condition","Deck - Mooring Machinery","Mooring","Equipment Related","9.2","Very High","","","Block overhauled and made operational","2020-12-06T23:59:35","","Completed","2020-11-30T23:59:35","No","No","No","Internal"]
[null,null,null,15739,null,"24_15/12/2020 10:46:24 PM","2020-11-28T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Few gratings on both port and stbd manifold valve operating stand is wasted","Deck - Pipe / Fittings","General Appearance","Equipment Related","6.6","Medium","","","Wasted grating sections renewed","2020-12-19T23:59:35","","Completed","2020-12-08T23:59:35","No","No","No","Internal"]
[null,null,null,15740,null,"24_15/12/2020 7:13:48 AM","2020-11-30T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Noted during routine testing of phones, workshop phone was not so audible and the keypad was also worn out. Also emergency DG room phone was also not so audible.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","All phone sets checked and tested. Defective phone set in emgcy dg room renewed, steering gear room phone cable renewed.","2020-12-31T23:59:35","","Completed","2020-12-14T23:59:35","No","No","No","Internal"]
[null,null,null,15421,null,"24_01/12/2020 9:03:40 AM","2020-12-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Two nos manual hand pumps for forward mooring winches inoperational","Deck - Mooring Machinery","Mooring","Equipment Related","9.14","Medium","","","Pumps overhauled and made operational.","2021-03-01T23:59:35","","Completed","2021-02-02T23:59:35","No","No","No","Internal"]
[null,null,null,14257,null,"24_15/10/2020 9:11:48 PM","2020-12-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Brake nut for mooring winch M4 cracked while tightening of brakes during random winch brake testing.","Deck - Mooring Machinery","Mooring","Equipment Related","9.14","Medium","","","Reqn DBAU200189 has been raised for spare brake nut. Temporary arrangement fabricated in place of brake nut. Job listed in DD specs. vessel in shipyard - to be attended in due time","2021-03-01T23:59:35","DBAU200189","Completed","2021-02-21T23:59:35","Yes","No","No","Internal"]
[null,null,null,15743,null,"24_15/12/2020 6:59:20 AM","2020-12-04T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Noted AE start air supply common line safety valve lifting sometimes - pressure reducing valve 30/10 k malfunction ","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Both pressure reducing valves 30/10K opened one by one and inspected parts. valve seat rubber found worn/damaged. one replaced with spare overhauled. the other one replaced with fabricated with rubber gasket. tested and found working satisfactory.","2021-01-11T23:59:35","","Completed","2020-12-19T23:59:35","No","No","No","Internal"]
[null,null,null,15744,null,"24_16/12/2020 10:39:01 AM","2020-12-05T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Cable counter for both windlasses not operational.","Deck - Machinery","General Appearance","Equipment Related,Inappropriate Procedure","9.2","Very High","","","Both cable counter gears to check and rectifiy. Job added to Refman list for attendance in DD.","2021-03-05T23:59:35","","Completed","2021-01-11T23:59:35","Yes","No","No","Internal"]
[null,null,null,15745,null,"24_15/12/2020 10:42:57 PM","2020-12-05T23:59:35","Defect","Ship Staff","Ship Staff Insp.","IG line drain pipe in china passage seems choked and drain valve is hard to operate.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related,Inappropriate Procedure","8.3","Very High","","","Pipeline choke cleared and valve eased up","2020-12-12T23:59:35","","Completed","2020-12-09T23:59:35","No","No","No","Internal"]
[null,null,null,15929,null,"24_20/12/2020 5:52:27 AM","2020-12-08T23:59:35","Defect","Ship Staff","Ship Staff Insp.","While preparing for hotwork, noted that the spare welding cable insulation had degraded and cracking at many places","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","5.25","Medium","","","old cable discarded and connectors removed it. A new cable prepared with the connectors and made ready for hotwork.","2020-12-08T23:59:35","","Completed","2020-12-08T23:59:35","No","No","No","Internal"]
[null,null,null,15928,null,"24_20/12/2020 5:33:35 AM","2020-12-09T23:59:35","Defect","Ship Staff","Ship Staff Insp.","AE 2 unit 5 and AE 3 unit 6 fuel cams found with fatique wear during camshafts inspections","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","To renew the camshaft sections with shore assistance. meanwhile polished the surface of affected cams and changed the respective rollers. Job added to Refman list for DD attendance","2021-03-09T23:59:35","DBAU210010","Completed","2021-01-15T23:59:35","Yes","No","No","Internal"]
[null,null,null,15418,null,"24_17/11/2020 10:08:40 AM","2020-12-11T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Stbd provision crane - condition of balance valve quite corroded and the limit valve for luffing/slewing circuit is not working, Noise from Flange bearings of jib hinge during luffing.","Deck - Machinery","General Appearance","Equipment Related","8.41","Medium","","","To replace the valves, flange bearing, RO raised for new ones. Job added to Refman for attendance in DD","2021-03-11T23:59:35","DBAU200226, DBAU210067","Completed","2021-01-11T23:59:35","No","No","No","Internal"]
[null,null,null,15419,null,"24_17/11/2020 10:59:09 AM","2020-12-11T23:59:35","Defect","Ship Staff","Ship Staff Insp.","ME alpha lubricator UPS noted in alarm condition and cooling fan not functional","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","ME alpha lub UPS battery and fan renewed with spare","2021-03-11T23:59:35","DBAU200229","Completed","2021-04-27T23:59:35","No","No","No","Internal","Old RO no. mentioned, Pls raise new if not done."]
[null,null,null,16553,null,"24_31/12/2020 11:27:45 AM","2020-12-12T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Low insulation alarm from ESBD for 220 V","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Investigated and found low insulation fault accomdation outside lights circuit breaker no. 22 on ESBD. All lights being checked one by one. found moisture in few fittings. sealing areas on fixture for cover being cleaned sealing rubber checked. Lights are also being coverted to LED fault is intermittent. all faults rectified.","2020-12-28T23:59:35","","Completed","2020-12-28T23:59:35","No","No","No","Internal"]
[null,null,null,15742,null,"24_16/12/2020 10:43:40 AM","2020-12-13T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Port windlass fwd operating lever block not operational.","Deck - Mooring Machinery","Mooring","Equipment Related","9.2","Very High","","","Block opened and checked, pilot piston missing on one end and cam in damaged condition. Spares ordered - renewed in DD","2021-03-13T23:59:35","DBAU210090","Completed","2021-03-12T23:59:35","No","No","No","Internal"]
[null,null,null,16556,null,"24_01/01/2021 4:28:07 PM","2020-12-13T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Pumproom gas detection system port side exhaust duct giving flow fault alarm","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related,External Factors","5.21","Medium","","","Port exhaust duct lines blown through and online filter inside pumproom and in ccr renewed and fault rectified","2020-12-16T23:59:35","","Completed","2020-12-15T23:59:35","No","No","No","Internal"]
[null,null,null,16554,null,"24_31/12/2020 4:56:50 PM","2020-12-14T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Meat room door heater faulty - ice built up","Accommodation,Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Checked and found door heater element faulty. RO raised for new element - renewed in DD","2021-03-14T23:59:35","DBAU210045","Completed","2021-03-13T23:59:35","No","No","No","Internal"]
[null,null,null,16555,null,"24_01/01/2021 3:16:56 PM","2020-12-14T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Two nos foam type fire extinguisher ring supports were found corroded.","LSA / FFA","Safety / LSA / FFA","Equipment Related,External Factors,Inappropriate Procedure","5.42","Medium","","","Corroded rings derusted and painted. ","2021-06-06T23:59:35","DBAU210001","Completed","2021-06-06T23:59:35","No","No","No","Internal","as per PAL RO supplied, Pls check.\nextending target date to close accordingly"]
[null,null,null,16557,null,"24_01/01/2021 2:59:27 PM","2020-12-14T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Two nos fire extinguihsher cradles base found corroded","LSA / FFA","Safety / LSA / FFA","External Factors","5.35","Medium","","","Cradles derusted and wasted base section cropper and renewed, paint applied and fitted back in location","2020-12-22T23:59:35","","Completed","2020-12-21T23:59:35","No","No","No","Internal"]
[null,null,null,14260,null,"24_16/10/2020 12:29:57 AM","2020-12-14T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Galley Oven door seal worn out","Accommodation","General Appearance","Equipment Related","11.13","Low","","","New seal ordered. Waiting for spares. Spares received and seal renewed.","2021-06-06T23:59:35","DBAU210007","Completed","2021-06-06T23:59:35","No","No","No","Internal","PO issued and awaiting delivery - to be delivered at next immediate suitable opportunity"]
[null,null,null,14388,null,"24_30/10/2020 11:12:51 PM","2020-12-16T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Few of the mooring winch brake cylinder clamping plates found wasted.","Deck - Mooring Machinery","Mooring","Equipment Related,External Factors","9.15","Medium","","","New brake cylinder clamping plates fabricated and fitted onto location","2021-02-16T23:59:35","","Completed","2021-01-28T23:59:35","No","No","No","Internal"]
[null,null,null,15741,null,"24_15/12/2020 6:53:20 AM","2020-12-16T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Noted jet assist air system not working during AE 1 starting. ","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","",""," Jet assist solenoid valve  renwed & working satisfactory.","2022-03-22T23:59:35"," DBAU210002","Completed","2022-01-12T23:59:35","No","No","No","Internal","RO was not followed up by vessel - Pls raise RO for complete unit, as there is no point in supplying al spares (which is almost comprises whole unit)."]
[null,null,null,14644,null,"24_15/11/2020 6:08:16 AM","2020-12-17T23:59:35","Defect","Ship Staff","Ship Staff Insp.","LO purifier no.2 control panel - running hour meter defective","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Running hour meter replaced by new one ","2021-10-22T23:59:35"," ","Completed","2021-09-01T23:59:35","No","No","No","Internal","Same old RO no. mentioned, as per PAL RO no. refers to deck lights"]
[null,null,null,14081,null,"24_30/09/2020 9:41:55 PM","2020-12-19T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Pumproom gas detection system air horn found damaged.","Miscellaneous","Cargo / Ballast Systems","Equipment Related","5.22","High","","","Temporary repairs carried out and horn made operational. Horn to be renewed. RO raised for new horn. Waiting for spares. Spare recieved. Renewed with new horn","2022-03-22T23:59:35","DBAU200204","Completed","2021-04-17T23:59:35","No","No","No","Internal","Already supplied - extending target date for completion"]
[null,null,null,17466,null,"24_15/01/2021 1:58:31 PM","2020-12-26T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Stbd lifeboat forward facing window faded with scratches.\t","LSA / FFA","Safety / LSA / FFA","Equipment Related,External Factors,Inappropriate Procedure","5.29","High","","","Scratched window replaced with clear acrylic sheet temporarily, to be replaced with tougned glass. Job added to Refman list. to get replacement toughned glass by giving acrylic sheet as sample in DD.","2021-02-19T23:59:35","","Completed","2021-01-16T23:59:35","Yes","No","No","Internal"]
[null,null,null,17475,null,"24_15/01/2021 1:47:35 PM","2020-12-26T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Chemical locker sprinkler valve found leaking","LSA / FFA","Safety / LSA / FFA","Equipment Related,Inappropriate Procedure","5.35","Medium","","","Valve replaced with onboard spare","2020-12-28T23:59:35","","Completed","2020-12-27T23:59:35","No","No","No","Internal"]
[null,null,null,17476,null,"24_16/01/2021 9:25:20 AM","2020-12-26T23:59:35","Defect","Ship Staff","Ship Staff Insp.","During furnace inspection noted some part of refractory in patially damaged condition.the metal plate at the gas outlet and on the garbage sluice drum has also partially burnt out. ","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Furnace cleaned, refractory patched up. Job added to Refman for permanent repairs in dry dock.","2020-12-27T23:59:35","","Completed","2020-12-27T23:59:35","Yes","No","No","Internal"]
[null,null,null,17467,null,"24_16/01/2021 9:34:42 AM","2020-12-27T23:59:35","Defect","Ship Staff","Ship Staff Insp.","During maintenance of FD fan vane control ring noted that control ring groves and vane ball pins are worn out. one of the vanes shaft was slightly loose","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","Vane control ring worn groove built up by welding. RO to be raised for new vane control ring, vane ball pins and vane shaft. ","2021-03-22T23:59:35","DBAU210029","Completed","2021-01-15T23:59:35","Yes","No","No","Internal"]
[null,null,null,17468,null,"24_16/01/2021 1:27:50 PM","2020-12-30T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Noted during ICCP checks as per maker's checklist, for Aft system 1,3 anodes performance not satisfactory, no.2 anode performance poor. For fwd system no .2 anode performance found poor.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Pre-checking sheet sent to maker for evaluation. To be atended in Drydock. Job added to Refman list for DD attendance","2021-03-22T23:59:35","","Completed","2021-01-15T23:59:35","Yes","No","No","Internal"]
[null,null,null,17469,null,"24_16/01/2021 1:32:22 PM","2020-12-31T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Noted AMS no.2 computer UPS battery condition alert light on","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Battery needs to be renewed. PO raised. Waiting for spares. Spare received and battery renewed.","2021-06-06T23:59:35","DBAU210009","Completed","2021-06-06T23:59:35","No","No","No","Internal","RO not followed by vessel, shall arrange at immediate opportunity"]
[null,null,null,17470,null,"24_15/01/2021 2:19:48 PM","2021-01-02T23:59:35","Defect","Ship Staff","Ship Staff Insp.","No.4S WBT sounding pipe holed near the deckhead penetration","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","Equipment Related,External Factors","11.7","High","","","Temporary repairs carried out. Job added to REFMAN for carrying out permanent repairs in drydock.","2021-03-02T23:59:35","","Completed","2021-01-11T23:59:35","Yes","No","No","Internal"]
[null,null,null,17477,null,"24_16/01/2021 1:38:51 PM","2021-01-02T23:59:35","Defect","Ship Staff","Ship Staff Insp.","VRCS pump station noted frequent high pressure alarm due to hyd pump unlading fault.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Adjusted the unloading pressure switch setting but not reliable as alarm started coming after some time again. Unloading pressure switch assembly renewed and fault rectified.","2021-01-05T23:59:35","","Completed","2021-01-04T23:59:35","No","No","No","Internal"]
[null,null,null,17471,null,"24_15/01/2021 2:38:03 PM","2021-01-03T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Port side no.2 manifold outer drain valve CL314 not holding during manifold integrity testing with compressed air.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related,External Factors","8.11","Medium","","","Valve seat ring to be renewed. RO to be raised for spare seat ring. Vessel awaiting spare seat ring.Tested during pressure testing of cargo lines. Valves integrity is holding","2022-02-19T23:59:35","DBAU210102","Completed","2021-09-10T23:59:35","No","No","No","Internal","RO was not followed up by vessel, will arrange at next immediate opportunity"]
[null,null,null,17478,null,"24_15/01/2021 2:36:15 PM","2021-01-03T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Port side no.1 manifold outer drain valve CL313 not holding during manifold integrity testing with compressed air.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related,External Factors","8.11","Medium","","","Valve dismantled, seat ring renewed. Integrity test carried out to 7bar pressure with compressed air and found to be holding.","2021-02-07T23:59:35","","Completed","2021-01-06T23:59:35","No","No","No","Internal"]
[null,null,null,17472,null,"24_16/01/2021 1:58:16 PM","2021-01-05T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Noted during low insulation fault finding that some of deck light fixtures are in deteriorated condition and insulation covering of wires inside the fixtures has degraded.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","",""," Low insulation fault rectified.","2021-06-21T23:59:35","DBAU210040, DBAU210041","Completed","2021-08-01T23:59:35","No","No","No","Internal","As per PAL, spares were supplied - Pls amend the remarks, extend target date if reqd"]
[null,null,null,17655,null,"24_31/01/2021 4:23:16 PM","2021-01-14T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Control air compressor delivery air flexible hose noted with minor leakage/seapage","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","control air comp replaced recently, old air hose reused. To be replaced new. RO raised.- replaced in DD","2021-03-14T23:59:35","DBAU210084","Completed","2021-03-13T23:59:35","No","No","No","Internal"]
[null,null,null,17658,null,"24_31/01/2021 4:32:33 PM","2021-01-14T23:59:35","Defect","Ship Staff","Ship Staff Insp.","IG fixed oxygen analyser no.1 - giving error 11 in all modes.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","error 11 investigated as per maker's instrcuctions, oxygen sensor replaced with new spare, checked all cable connection, but error persisted. analyser reciver needs to be replaced. RO raised for new one. - received and renewed in DD","2021-03-01T23:59:35","DBAU210069, DBAU215014","Completed","2021-03-13T23:59:35","No","No","No","Internal"]
[null,null,null,17659,null,"24_31/01/2021 4:37:31 PM","2021-01-14T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Noted during COPT alarms testing that remote emergency trip was not resetting for all 3 COPTs.","Cargo Mach.,Critical Equip.,Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Checked and found barrier unit malfunction. unit replaced with spare new one fault rectified. RO to be raised for new spares","2021-01-15T23:59:35","","Completed","2021-01-14T23:59:35","No","No","No","Internal"]
[null,null,null,17656,null,"24_01/02/2021 6:13:41 AM","2021-01-15T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Aux boiler no.1 FO temperature indicator controller alarm during UMS, indicator showing erratic reading, actual FO temp is correct.","E/R - Boiler,Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Indicator confirmed erratic by ETO, to be opened up for further checks/ rectification and to order new if required. - Checked and found loose internal contacts/connections. rectified, working satisfactory.","2021-02-15T23:59:35","","Completed","2021-02-04T23:59:35","No","No","No","Internal"]
[null,null,null,17657,null,"24_31/01/2021 4:44:43 PM","2021-01-17T23:59:35","Defect","Ship Staff","Ship Staff Insp.","During inspection/ checks on accomodation AC AHU unit performance, noted return air temp sensors were defective. Also the local dial thermoeters were not indicating correctly.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Sensors / thermometers need to be replaced for correct air temp control/ AC compressor operation. RO raised - received and replaced in DD","2021-03-16T23:59:35","DBAU210051","Completed","2021-03-13T23:59:35","No","No","No","Internal"]
[null,null,null,17824,null,"24_15/02/2021 5:32:35 PM","2021-01-24T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Noted IG O2 analyser sample line section with numerous cracks after the root valve from Main IG line - due to aging","E/R - Aux. Mach.,Inert Gas","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Temporary pipe used between the root valve and O2 analyser for the operations. original damaged section removed and replaced with new tube.","2021-01-31T23:59:35","","Completed","2021-01-26T23:59:35","No","No","No","Internal"]
[null,null,null,17821,null,"24_15/02/2021 5:38:36 PM","2021-01-25T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Steering gear LO transfer pump opened for repair of minor leak, also noted spider between pump and motor coupling in damaged condition. No PMS routines existing for the pump","E/R - Aux. Mach.,E/R - Pumps","Eng. / Strg. Comp.","Equipment Related,Human Error","10.32","Very High","","","Pump leak rectified, spider fabricated from teflon as no spare available, PMS routines added. RO raised for new spider - new spider received","2021-04-04T23:59:35","DBAU210085","Completed","2021-03-31T23:59:35","No","No","No","Internal"]
[null,null,null,17822,null,"24_15/02/2021 5:55:54 PM","2021-01-25T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Noted during discharge operation erratic auto operation of AUS with COP no. 1 & 2  ","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.8","Medium","","","COP no.2 discharge valve positioner found with damaged range adjuster causing erratic valve operation - valve positioner renewed and adjusted for full valve range. COP no.1 discharge valve positioner found with faulty range setting and valve position transmitter zero setting - both corrected. COP no.1 seperator level transmitter calibration checked and rough zero adjustment done. System to be checked during next discharge operation. AUS system components need to be checked/serviced in DD. Job added in Refman. found working satisfactorily during discharge operation on 18.02.2021","2021-04-04T23:59:35","","Completed","2021-02-10T23:59:35","Yes","No","No","Internal"]
[null,null,null,17826,null,"24_15/02/2021 6:07:08 PM","2021-01-25T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Noted during ME operation no. 3 unit not reversing some times, found minor air leak from the air connection of unit 3 reversing cylinder","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Air cylinder dismantled and found air connection threads on the cylinder cover in damaged condition (assuming happened during last overhaul job). air cylinder replaced with new spare set. ME tested and found workinf satisfactorily.","2021-02-01T23:59:35","","Completed","2021-01-26T23:59:35","No","No","No","Internal"]
[null,null,null,17823,null,"24_16/02/2021 2:27:34 AM","2021-01-26T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Four nos ballast tank gaugings system readings showing erratic readings","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.8","Medium","","","Job DK 57 has been added to REFMAN for servicing of the system.","2021-03-26T23:59:35","","Completed","2021-02-08T23:59:35","No","No","No","Internal"]
[null,null,null,17825,null,"24_17/02/2021 5:29:04 AM","2021-02-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","MGPS alarm received, found no output to Low sea chest anodes","E/R - Aux. Mach.,Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","control box opened and checked found power supply PCB/unit defective, temporary repair carried out on the PCB and made functional. RO raised for new spare PCB - to be repalced in DD","2021-02-08T23:59:35","","Completed","2021-02-04T23:59:35","Yes","No","No","Internal"]
[null,null,null,18098,null,"24_02/03/2021 9:42:06 AM","2021-02-09T23:59:35","Defect","Ship Staff","Ship Staff Insp.","No.3 COPT noted governor control from CCR erratic, control switch suspected","Cargo Mach.,E/R - Aux. Mach.,Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Control switch in CCR panel renewed and tested found satisfactory","2021-02-11T23:59:35","","Completed","2021-02-10T23:59:35","No","No","No","Internal"]
[null,null,null,18099,null,"24_02/03/2021 9:37:22 AM","2021-02-13T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Atm condenser minor SW leak detected via salinity sensor giving high alarm","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","condenser required to be pressure tested, identify source of leak and rectify. Job added to DD specs in consultation with office. Boiler and feed water salinity monitored and under control by boiler blowdowns","2021-03-21T23:59:35","","Completed","2021-02-15T23:59:35","No","No","No","Internal"]
[null,null,null,18731,null,"24_21/04/2021 2:37:54 PM","2021-03-23T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Both LT coolers end plates noted to be wasted iwo SW outlet","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","RO raised, received new plates without opening for filter bucket. Awaiting plate modification for hole. to be replaced once ready. Plate modification done & installed.","2022-03-22T23:59:35","NA","Completed","2022-02-25T23:59:35","No","No","No","Internal"]
[null,null,null,18729,null,"24_21/04/2021 2:42:39 PM","2021-03-24T23:59:35","Defect","Ship Staff","Ship Staff Insp.","LO purifier no.1 heater - noted leak during hyd pressure test in yard workshop","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","new heater ordered, to be replaced when received. New heater received and has been replaced on purifier no.1.","2021-05-21T23:59:35","DBAU215090","Completed","2021-05-04T23:59:35","No","No","No","Internal"]
[null,null,null,18726,null,"24_21/04/2021 12:22:46 PM","2021-04-03T23:59:35","Defect","Ship Staff","Ship Staff Insp.","FPK tank valve BA422 & 1S main valve BA402 leaking.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.11","Medium","","","   1S and fore peak valve found holding good.  Only manual hydraulic valve BA401 has to be confirmed fully tight shut.  ","2022-02-19T23:59:35","","Completed","2022-09-19T23:59:35","Yes","No","No","Internal","Please update the status of this defect."]
[null,null,null,18727,null,"24_21/04/2021 2:58:10 PM","2021-04-06T23:59:35","Defect","Ship Staff","Ship Staff Insp.","AE sump oil seemed contaminated with LSMGO by appearance","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Viscosity has reduced, checks done - suspected plunger barrels (21000rhrs) as reason for the minor leakage during operation in LSMGO. All pumps to be overhauled with new plunger barrel sets, avaialble onboard. Sump oil renewed, AE on FO standby.All fuel pumps overhauled with new plunger barrel assembly","2021-06-21T23:59:35","","Completed","2021-05-28T23:59:35","No","No","No","Internal"]
[null,null,null,18728,null,"24_21/04/2021 3:05:58 PM","2021-04-06T23:59:35","Defect,Guarantee Claim","Ship Staff","Ship Staff Insp.","BWTS defects – 1) faulty salinity & temp sensor on the feed water line to electrolysis unit. 2) MCC-100 Cabinet temp high alarm  3) no.3 filter FCV feed back sensor fault alarm  ","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","",""," Attended by technician and fault rectified","2021-12-22T23:59:35","","Completed","2021-10-04T23:59:35","No","No","No","Internal"]
[null,null,null,18730,null,"24_21/04/2021 12:30:33 PM","2021-04-11T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Deck seal drain pipe holed","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.25","Very High","","","Deck seal drain pipe renewed.","2021-06-21T23:59:35","","Completed","2021-06-06T23:59:35","No","No","No","Internal"]
[null,null,null,19273,null,"24_29/04/2021 6:01:27 AM","2021-04-13T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Noted cooling fan not running and equipment not in working condition","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","To check and revert if any issues – to repair earliest as Control air is critical. Control air compressor is running with auto drain system modified. Cooling fan repaired and is working now.","2021-06-06T23:59:35","","Completed","2021-05-31T23:59:35","No","No","No","Internal","Target date amended - as the Obs list was sent to vessel a week later than the obs made date"]
[null,null,null,19274,null,"24_29/04/2021 6:14:05 AM","2021-04-13T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Few lagging observed damaged and worn","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Damaged insulation/lagging replaced","2021-04-23T23:59:35","","Completed","2021-04-23T23:59:35","No","No","No","Internal","Target date amended - as the Obs list was sent to vessel a week later than the obs made date"]
[null,null,null,19275,null,"24_29/04/2021 6:18:04 AM","2021-04-13T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Hour meter display unit observed flickering","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Hour meter to be checked. Hour meter renewed.","2021-06-06T23:59:35","","Completed","2021-06-06T23:59:35","No","No","No","Internal","Target date amended - as the Obs list was sent to vessel a week later than the obs made date"]
[null,null,null,19276,null,"24_29/04/2021 6:21:43 AM","2021-04-13T23:59:35","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","AC compressor - Save all tray oily/dirty ","E/R - Aux. Mach.","General Appearance","Equipment Related","10.32","Very High","","","Cleaning of save-all completed","2021-04-29T23:59:35","","Completed","2021-04-29T23:59:35","No","No","No","Internal"]
[null,null,null,19277,null,"24_29/04/2021 6:24:29 AM","2021-04-13T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Aux Boiler - Feed water lines behind boiler found few laggings damaged","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Renewal of lagging/insulation completed","2021-05-02T23:59:35","","Completed","2021-04-29T23:59:35","No","No","No","Internal"]
[null,null,null,19278,null,"24_29/04/2021 6:32:43 AM","2021-04-13T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Port blr-found tube light near water transmitter fused","Elect. Mach. & Equip.","General Appearance","Equipment Related","10.37","Medium","","","Fused tube replaced and is working ","2021-04-14T23:59:35","","Completed","2021-04-14T23:59:35","No","No","No","Internal","Target date amended - as the Obs list was sent to vessel a week later than the obs made date"]
[null,null,null,19279,null,"24_29/04/2021 6:44:09 AM","2021-04-13T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Space dirty – after works at DD","E/R - Pumps","Eng. / Strg. Comp.","Behaviour Based","10.32","Very High","","","Cleaning  completed, painting in progress.","2021-06-21T23:59:35","","Completed","2021-08-05T23:59:35","No","No","No","Internal","Target date amended - as the Obs list was sent to vessel a week later than the obs made date"]
[null,null,null,19280,null,"24_29/04/2021 6:50:03 AM","2021-04-13T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Emergency hand pump in sterring gear Port side pump level gauge fitted upside down","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","To investigate and rectify. Level gauge fitted correctly.","2021-05-22T23:59:35","","Completed","2021-05-05T23:59:35","No","No","No","Internal"]
[null,null,null,19281,null,"24_29/04/2021 6:54:44 AM","2021-04-13T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Steering gear room - HHC Lying loose not identified and tagged","E/R - Aux. Mach.","Eng. / Strg. Comp.","Human Error","10.32","Very High","","","To ensure they are separated and kept, identifying with the relevant crane’s spares. Hoses identified and stored properly","2021-05-13T23:59:35","","Completed","2021-05-12T23:59:35","No","No","No","Internal"]
[null,null,null,19282,null,"24_29/04/2021 6:59:14 AM","2021-04-13T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","EGCS chemical solution - Buffer solutions lying open and discarded","Miscellaneous","Eng. / Strg. Comp.","Human Error","10.32","Very High","","","Buffer solution drums shifted to chemical locker and secured.","2021-04-29T23:59:35","","Completed","2021-04-27T23:59:35","No","No","No","Internal"]
[null,null,null,19283,null,"24_29/04/2021 7:02:26 AM","2021-04-13T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","EGCS SW inlet pipe in steering gear room - The light was in an inappropriate location fouling with actuator- to relocate","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Human Error","10.37","Medium","","","Light fixture relocated and fitted.","2022-03-22T23:59:35","NA","Completed","2022-02-19T23:59:35","No","No","No","Internal"]
[null,null,null,19284,null,"24_29/04/2021 7:06:40 AM","2021-04-13T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","440V - Panel showing low insulation panel – suspect from Icolube panel?","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.38","Medium","","","Insulation fault traced and rectified.","2021-05-06T23:59:35","","Completed","2021-05-04T23:59:35","No","No","No","Internal","Target date amended - as the Obs list was sent to vessel a week later than the obs made date"]
[null,null,null,19285,null,"24_29/04/2021 7:21:56 AM","2021-04-13T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ME FO circulating pump - Oil drop sighted (leaks)","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.12","Very High","","","Pump to be overhauled if leak is from mechanical seal. No leak observed from either mechanical seal or from flange/gaskets. Pump is kept under observation.","2021-05-08T23:59:35","","Completed","2021-05-05T23:59:35","No","No","No","Internal"]
[null,null,null,19286,null,"24_29/04/2021 7:24:57 AM","2021-04-13T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Ship Staff Insp.","Service air compressor - Not in operation – understand unloader defective","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Unloader changed with new received spare, now service air compressor is working satisfactory.","2021-10-21T23:59:35","","Completed","2021-10-07T23:59:35","No","No","No","Internal"]
[null,null,null,19287,null,"24_29/04/2021 7:33:32 AM","2021-04-13T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","AE No.2 - Lot of LO leaks observed aft of Engine – dabbas/containers kept","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Various leaks are being attended to. All leaks arrested","2021-05-22T23:59:35","","Completed","2021-05-16T23:59:35","No","No","No","Internal"]
[null,null,null,19288,null,"24_29/04/2021 8:01:28 AM","2021-04-13T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","New Sewage Holding tank - Tank capacity not stencilled","Hull & Tanks","Eng. / Strg. Comp.","Human Error","10.32","Very High","","","Tank capacity to be stencilled. Tank stencilled.","2021-05-06T23:59:35","","Completed","2021-05-05T23:59:35","No","No","No","Internal"]
[null,null,null,19289,null,"24_29/04/2021 8:04:11 AM","2021-04-13T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ME - Save all spaces – cylinder heads, fuel pumps, dirty","E/R - Main Engine","General Appearance","Human Error","10.32","Very High","","","To soap wash ME cylinder head,fuel pumps and their save-alls - Job in progress. Job completed","2021-05-13T23:59:35","","Completed","2021-05-12T23:59:35","No","No","No","Internal"]
[null,null,null,19290,null,"24_29/04/2021 8:08:22 AM","2021-04-13T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ER - Cosmetically dirty after upgrade works at ship yard","E/R - Air Comp.,E/R - Aux. Engine,E/R - Aux. Mach.,E/R - Boiler,E/R - Main Engine,E/R - Pipes/ valves & fittings,E/R - Pumps,E/R - Purifier","Eng. / Strg. Comp.","Human Error","10.32","Very High","","","Engine Room cleaning completed, painting in progress  ","2021-06-21T23:59:35","","Completed","2021-08-05T23:59:35","No","No","No","Internal"]
[null,null,null,19291,null,"24_29/04/2021 8:22:06 AM","2021-04-13T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ODME - Pump passing thru ER b/head, the lubricator pail is dark and not visible of oil is there are not","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Pail cleaned and oil topped-up ","2021-04-24T23:59:35","","Completed","2021-04-24T23:59:35","No","No","No","Internal","Target date amended - as the Obs list was sent to vessel a week later than the obs made date"]
[null,null,null,19292,null,"24_29/04/2021 8:25:07 AM","2021-04-13T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ME - New bearings and old ones are mixed up and kept in COPT platform","E/R - Main Engine","Eng. / Strg. Comp.","Inappropriate Procedure","10.32","Very High","","","ME bearings to be properly stowed in separate boxes. ME bearings segregated. Old bearings put in a separate box for landing ashore at next call Singapore","2021-05-22T23:59:35","","Completed","2021-05-06T23:59:35","No","No","No","Internal"]
[null,null,null,19293,null,"24_29/04/2021 8:27:53 AM","2021-04-13T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","OWS - Exterior housing dirty","E/R - Aux. Mach.","General Appearance","Human Error","10.32","Very High","","","OWS cleaned and painted.Operational readiness checked as pumped out BHT.","2021-04-24T23:59:35","","Completed","2021-04-24T23:59:35","No","No","No","Internal","Target date amended - as the Obs list was sent to vessel a week later than the obs made date"]
[null,null,null,19294,null,"24_29/04/2021 8:30:59 AM","2021-04-13T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ME - Air leaks observed near #7 fuel pump solenoid valve block","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","ME pneumatic control system valve no.321 needs to check and overhaul when engine is not running. Valve no 321 overhauled and leak rectified","2021-05-28T23:59:35","","Completed","2021-05-27T23:59:35","No","No","No","Internal"]
[null,null,null,19295,null,"24_29/04/2021 8:41:37 AM","2021-04-13T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","BWTS - #3 Filter flow control valve feed back sensor defective","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Rectified by BWTS Technician","2021-10-22T23:59:35","","Completed","2021-10-04T23:59:35","No","No","No","Internal","Target date amended - as the Obs list was sent to vessel a week later than the obs made date"]
[null,null,null,19296,null,"24_29/04/2021 8:45:59 AM","2021-04-13T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","BWTS - Ventilation not sufficient for rectifier/control and filter units","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","To modify/re-route ventilation ducts accordingly. Ventilation duct fabricated and rerouted.","2021-06-06T23:59:35","","Completed","2021-05-29T23:59:35","No","No","No","Internal"]
[null,null,null,19297,null,"24_29/04/2021 8:52:43 AM","2021-04-13T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","EGCS - Top bracing bolts passes across access paltform","E/R - Aux. Mach.","Safety / LSA / FFA","Human Error","10.15","Low","","","Trip hazard – to fabricate crossover walkways. Cross-over walkway fabricated and fitted","2021-06-13T23:59:35","","Completed","2021-05-29T23:59:35","No","No","No","Internal"]
[null,null,null,19298,null,"24_29/04/2021 8:48:45 AM","2021-04-13T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","SGCS - CE reported that drain valve positioner beeter to keep as spare","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","To check, verify and if required to raise RO. No need to keep this valve as spare.","2021-05-06T23:59:35","","Completed","2021-05-04T23:59:35","No","No","No","Internal"]
[null,null,null,19299,null,"24_29/04/2021 8:58:14 AM","2021-04-13T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","EGCS - Bracing bolts, tie stids some nuts were found loose","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.15","Low","","","all lock nuts tightness checked and tightened. ","2021-04-29T23:59:35","","Completed","2021-04-29T23:59:35","No","No","No","Internal"]
[null,null,null,19300,null,"24_29/04/2021 9:05:02 AM","2021-04-13T23:59:35","Critical Equipment","Owner / Marine / Tech. Suptd.","Suptd. Insp.","EGCS - No fire extinguishers anywhere","LSA / FFA","Eng. / Strg. Comp.","Human Error","5.42","Medium","","","All fire extinguishers are in place","2021-04-26T23:59:35","","Completed","2021-04-26T23:59:35","No","No","No","Internal"]
[null,null,null,19301,null,"24_29/04/2021 10:29:14 AM","2021-04-13T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","EGCS Housing - Top platform access door not locked and tower access door no security tags","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.15","Low","",""," bottom access door locked and 1 set of keys in ECR and 1 in CCR – top door  locked and security tag  installed form outside","2021-05-11T23:59:35","","Completed","2021-05-23T23:59:35","No","No","No","Internal","Target date amended - as the Obs list was sent to vessel a week later than the obs made date"]
[null,null,null,19302,null,"24_29/04/2021 10:37:00 AM","2021-04-13T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Aux Boiler - Remote valve release wires not free and not activating","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Remote valve release wires freed and made operational.","2021-04-24T23:59:35","","Completed","2021-04-24T23:59:35","No","No","No","Internal","Target date amended - as the Obs list was sent to vessel a week later than the obs made date"]
[null,null,null,19303,null,"24_29/04/2021 10:39:38 AM","2021-04-13T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Exhaust uptakes lagging – found few not applied fully and new lagging just placed on the pipes","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Laggings received in Singapore and applied on exhaust uptakes.","2021-06-21T23:59:35","","Completed","2021-06-07T23:59:35","No","No","No","Internal"]
[null,null,null,19304,null,"24_30/04/2021 8:58:00 PM","2021-04-13T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","M5 mooring winch brake cylinder reported leaking.","Deck - Mooring Machinery","Mooring","Equipment Related","9.1","Low","","","BRAKE CYLINDER VAVLE BLOCK ORING CHANGED, LEAK RECTIFIED.","2021-05-18T23:59:35","","Completed","2021-05-14T23:59:35","No","No","No","Internal"]
[null,null,null,19305,null,"24_30/04/2021 9:02:59 PM","2021-04-13T23:59:35","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","hose handling crane hoses kept in midship store without identification.","Deck - Machinery","Cargo / Ballast Systems","Behaviour Based","8.5","Very High","","","ALL HYDRAULIC HOSES FOR CARNE SORTED OUT AND KEPT IN STEERING GEAR ROOM.","2021-06-13T23:59:35","","Completed","2021-05-23T23:59:35","No","No","No","Internal"]
[null,null,null,19306,null,"24_30/04/2021 9:07:38 PM","2021-04-13T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Most of the markings on deck  were faded after repairs at ship yard","Deck - Pipe / Fittings","General Appearance","External Factors","8.6","Medium","",""," Stenciling completed","2021-07-13T23:59:35","","Completed","2021-08-05T23:59:35","No","No","No","Internal"]
[null,null,null,19307,null,"24_30/04/2021 9:10:35 PM","2021-04-13T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","#5 Fire hose box on deck upper lock damaged","LSA / FFA","Safety / LSA / FFA","Equipment Related","10.1","Medium","","","#5 FIRE HOSE SECURING ARRANGEMENT RENEWED.","2021-06-21T23:59:35","","Completed","2021-05-22T23:59:35","No","No","No","Internal"]
[null,null,null,19308,null,"24_30/04/2021 9:12:50 PM","2021-04-13T23:59:35","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Vessel does not have mini blaster for pipes under sides maintenance ","Miscellaneous","General Appearance","Equipment Related","","","","","RO RAISED DBAU210137","2021-05-22T23:59:35","","Completed","2021-05-22T23:59:35","No","No","No","Internal"]
[null,null,null,19309,null,"24_30/04/2021 9:15:59 PM","2021-04-13T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Foam monitor-Turrent springs were found rusted at various stages","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.35","Medium","","",".RO raised DBAU210143 for springs","2021-06-13T23:59:35","","Completed","2021-06-07T23:59:35","No","No","No","Internal"]
[null,null,null,19310,null,"24_30/04/2021 9:20:20 PM","2021-04-13T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Mooring winches brake band stopper bolt were found clearances either excessive or less .","Deck - Mooring Machinery","Mooring","Equipment Related","9.2","Very High","","","mOORING WINCHES STOPPER BOLT ADJUSTED TO CLEARENCE LESS THAN 3 MM","2021-06-11T23:59:35","","Completed","2021-05-22T23:59:35","No","No","No","Internal"]
[null,null,null,19311,null,"24_30/04/2021 9:25:14 PM","2021-04-13T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","1S,2P, 3P,3S, 4P & 4S WBT Hanla Electro-Pneumatic level gauge showing  erratic readings.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.1","Very High","","","1.\tWe have checked free passage of the air line by water blowing, followed by air blowing the line, Caliberated the Zero and Span setting by pressure caliberator as per procedure in manual and size of the tank.\n2.\tObserved the Draft gauges to show accurate,\n3.\t3S,4 & 5 Ballast tanks reading are working satisfactory,\n4.\t2P Tank was working satisfactory but presently showing full reading due to blockage of line from deck to the tank, To clear the same at convenient opportunity,\n5.\t1P, 2S Air lines were blanked on top of the ballast tank and observed the reading to show full in the tank indicator, The lines are leaking inside the tank hence shows empty/Partial,\n6.\tFP, APT, 3P ballast tank Air line from the upper deck to Tank top is leaking, to identify the leak and rectify,\n7.\t1S Ballast tank is found to have mild leakage due to which the level does not show beyond 25M, To check for mild leak and rectify.\n8. Futher investigation to be carried out during load passage as ballast tanks will be empty.\n All lines, pressure transmitter checked for integrity and proper working. Dead sounding for the ballast tanks calibrated. Will check during ballasting operation at discharge port.\nGauges still not operational after servicing in drydock, have sent msg to superintendent and awaiting feedback.\nClosed out.","2024-06-29T23:59:35","DBAU220181","Completed","2023-03-01T23:59:35","No","No","No","Internal","SE attended the vessel in Singapore in August 2022. Spares have been ordered but vessel is yet to complete complete investigation.  Please carry out complete investigation during loaded passage and revert with findings. Spares have been raised."]
[null,null,null,19312,null,"24_30/04/2021 9:56:31 PM","2021-04-13T23:59:35","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Both Deck and Engine room , need lot of cleaning and squaring up at various locations – as the most of the spaces are dirtyafter ship yard repairs","Accommodation,Deck - Pipe / Fittings,Miscellaneous","General Appearance","External Factors","10.29","Medium","","","All stores , common areas , cleaning gear lockers , deck & E/R cleaned and arranged.","2021-06-13T23:59:35","","Completed","2021-06-05T23:59:35","No","No","No","Internal"]
[null,null,null,19313,null,"24_29/04/2021 6:38:58 AM","2021-04-13T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Steering gear-fire doors were kept open","Miscellaneous","Eng. / Strg. Comp.","Behaviour Based","10.44","Medium","","","lashing removed and doors closed in good order","2021-04-13T23:59:35","","Completed","2021-04-13T23:59:35","No","No","No","Internal"]
[null,null,null,19314,null,"24_29/04/2021 7:15:41 AM","2021-04-13T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Dep checklist – Shekou – noticed ICCP power ticked as ON, when it was not in use during the Voyage","Documentation","Eng. / Strg. Comp.","Inappropriate Procedure","10.5","Low","","","Checklist amended.","2021-04-19T23:59:35","","Completed","2021-04-19T23:59:35","No","No","No","Internal"]
[null,null,null,19315,null,"24_29/04/2021 7:18:29 AM","2021-04-13T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Arr Singapore checklist not sighted","Documentation","Eng. / Strg. Comp.","Inappropriate Procedure","10.5","Low","","","Checklist filled and updated","2021-04-19T23:59:35","","Completed","2021-04-19T23:59:35","No","No","No","Internal"]
[null,null,null,19316,null,"24_29/04/2021 7:30:53 AM","2021-04-13T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Emergency escape - Found all lights off – circuit tripped?","Elect. Mach. & Equip.","Emgcy. Systems","Human Error","10.37","Medium","","","Lights made operational","2021-04-19T23:59:35","","Completed","2021-04-19T23:59:35","No","No","No","Internal"]
[null,null,null,19317,null,"24_29/04/2021 8:18:41 AM","2021-04-13T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","PPE kept neat Boiler feed pump – eyewash expired, no complete PPE","LSA / FFA","Eng. / Strg. Comp.","Human Error","5.5","Low","","","PPE checked and replenished.","2021-04-19T23:59:35","","Completed","2021-04-19T23:59:35","No","No","No","Internal"]
[null,null,null,19318,null,"24_29/04/2021 8:35:10 AM","2021-04-13T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","EGCS - Sea water pump motor reported running temps were high","E/R - Pumps,Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Pump motor checked. Found to be normal as temperature rises with respect to rise in ambient temperature.","2021-04-20T23:59:35","","Completed","2021-04-20T23:59:35","No","No","No","Internal"]
[null,null,null,19319,null,"24_29/04/2021 10:32:50 AM","2021-04-13T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Port side boiler - found water level not matching with both gauge glasses","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Blow down of gauge glass carried out and checked. Level found satisfactory","2021-04-19T23:59:35","","Completed","2021-04-19T23:59:35","No","No","No","Internal"]
[null,null,null,19320,null,"24_29/04/2021 8:10:47 AM","2021-04-13T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ME alpha LO pump save-all - Observed oil in save all of pump ","E/R - Pumps","Eng. / Strg. Comp.","Human Error","10.32","Very High","","","Save-all cleaned. ","2021-04-19T23:59:35","","Completed","2021-04-19T23:59:35","No","No","No","Internal"]
[null,null,null,20302,null,"24_16/07/2021 7:10:54 PM","2021-04-16T23:59:35","Defect","Ship Staff","Ship Staff Insp.","No.1 EGCS Pump( stbd) mechanical seal leakage","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","New Mechanical seal received and pump was overhauled with new mechanical. Pump tried out, now working without any leakage from mechanical seal.","2021-07-15T23:59:35","","Completed","2021-06-22T23:59:35","No","No","No","Internal"]
[null,null,null,19385,null,"24_08/05/2021 3:38:54 PM","2021-04-29T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Both Hose handling crane limit switch assembly complete with gear box found to be in-operational as reduction gear teeth were found to be broken","Deck - Machinery","Safety / LSA / FFA","Equipment Related","8.63","High","","","Port hose handling crane limit switche replaced with new recieved spare and stbd hose handling crane limit switch replaced with repaired limit switch, not both cranes limits are working properly.","2021-06-21T23:59:35","DBAU210124","Completed","2021-06-20T23:59:35","No","No","No","Internal"]
[null,null,null,19581,null,"24_18/5/2021 4:50:49 AM","2021-05-08T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Stbd bridge wing gyro repeater dimmer switch not operational.","Navigation - Others","Navigation","Equipment Related","","","","","Fused bulb renewed by ETO.","2021-08-07T23:59:35","","Completed","2021-06-05T23:59:35","No","No","No","Internal"]
[null,null,null,19582,null,"24_18/5/2021 4:54:59 AM","2021-05-08T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Bridge wing doppler log repeaters on both side, dimmer switch not opeartional. Even during daytime the screen appears smudged and is not easy to read.","Navigation - Echo Sounder / Speed Log","Navigation","Equipment Related","","","","","Bridge wing Port & Stbd  Display PCB replaced by new one.","2021-10-22T23:59:35","DBAU210131","Completed","2021-10-06T23:59:35","No","No","No","Internal"]
[null,null,null,19583,null,"24_30/05/2021 7:02:38 PM","2021-05-21T23:59:35","Observation","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","Both L/Boat sea water cooling lines were painted over thus reducing the cooling effect.","LSA / FFA","Safety / LSA / FFA","Human Error","5.28","Very High","","","PAINT REMOVED FROM SEA WATER COOLING LINE OF PORT AND STBD LIFEBOATS.","2021-05-27T23:59:35","","Completed","2021-05-24T23:59:35","No","No","No","External"]
[null,null,null,19584,null,"24_30/05/2021 7:10:25 PM","2021-05-21T23:59:35","Observation","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","Lathe Machine in engine room workshop was found without chuck protector","Miscellaneous","Eng. / Strg. Comp.","Human Error","10.27","Medium","","","Need to fabricate one and fitted. Chuck guard fabricated and fitted","2021-06-01T23:59:35","","Completed","2021-05-24T23:59:35","No","No","No","External"]
[null,null,null,19585,null,"24_31/05/2021 11:19:16 AM","2021-05-22T23:59:35","Critical Equipment","Ship Staff","Ship Staff Insp.","PORT L/BOAT ENGINE IS NOT ENGAGING PROPERLY IN AHEAD & ASTERN PROPULSION","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.29","High","","","NEED TO CHECK THE ENGAGING GEAR ASSEMBLY.  ENGAGING SYSTEM CHECKED. WORKING FINE","2021-05-31T23:59:35","","Completed","2021-05-28T23:59:35","No","No","No","Internal"]
[null,null,null,19586,null,"24_31/05/2021 12:16:18 PM","2021-05-22T23:59:35","Critical Equipment","Ship Staff","Ship Staff Insp.","One Fire Line Isolation valve on fwd maine deck found very hard to open/close by hand.","LSA / FFA","Safety / LSA / FFA","Human Error","5.38","High","","","ISOLATION VAVLE OVERHAULED AND MADE FREE AND LUBRICATED.","2021-05-29T23:59:35","","Completed","2021-05-25T23:59:35","No","No","No","Internal"]
[null,null,null,19587,null,"24_01/06/2021 10:54:09 PM","2021-05-22T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Drop Valve No 250 & 251 hydraulic lines were found leaking in 3C COTK.","Deck - Pipe / Fittings","Cargo / Ballast Systems","External Factors","8.11","Medium","","","Detailed investigation carried out.Oil level in hydraulic tank monitotred,no drop of oil level observed.Both drop valves operated during loading operation at DAS ISLAND.No leak observed.","2021-07-27T23:59:35","","Completed","2021-06-18T23:59:35","No","No","No","Internal"]
[null,null,null,20303,null,"24_16/07/2021 7:04:47 PM","2021-06-03T23:59:35","Defect","Ship Staff","Ship Staff Insp.","No.1 Ballast pump upper bearing tempearture is high","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.8","Medium","","","Bo.1 Ballast pump overhauled with new ball bearing, bearing housing, flinger , locking washer and locking nut. Pump tried out, upper bearing temperature found within normal range.","2021-09-02T23:59:35","","Completed","2021-07-06T23:59:35","No","No","No","Internal"]
[null,null,null,20290,null,"24_01/07/2021 1:39:33 PM","2021-06-04T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Observed hydraulic oil leakgae at control pipe connection for high/low speed operating lever for stbd windlass.","Deck - Mooring Machinery","Mooring","Equipment Related","9.1","Low","","","Leakage rectified.","2021-10-22T23:59:35","","Completed","2021-08-28T23:59:35","No","No","No","Internal"]
[null,null,null,20291,null,"24_14/7/2021 5:23:08 PM","2021-06-11T23:59:35","Observation","Ship Staff","Nav Audit / Verification","One window wiper not operational","Navigation - Others","Navigation","Equipment Related","12.1","High","","","Fault rectified","2021-09-10T23:59:35","","Completed","2021-08-03T23:59:35","No","No","No","Internal"]
[null,null,null,20292,null,"24_14/7/2021 5:29:28 PM","2021-06-11T23:59:35","Defect","Ship Staff","Nav Audit / Verification","Port side Search light locking arrangement for particular postion broken.","Navigation - Others","Navigation","Equipment Related","","","","","Repaired.","2022-01-22T23:59:35","","Completed","2021-12-30T23:59:35","No","No","No","Internal"]
[null,null,null,20293,null,"24_13/7/2021 9:58:06 PM","2021-06-23T23:59:35","Defect","Ship Staff","Ship Staff Insp.","NO 2 cargo oil eductor not taking suction, cargo flows back to suction tank.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.8","Medium","","","to be investigated and rectified.\nFound both cargo eductor  working correctly during last cargo discharge operation .","2022-03-22T23:59:35","","Completed","2022-10-27T23:59:35","No","No","No","Internal","I believe the cargo eductor is working fine and no issues have been reported. Please update and close out the defect accordingly."]
[null,null,null,20294,null,"24_15/07/2021 3:35:14 PM","2021-06-23T23:59:35","Defect","Ship Staff","Ship Staff Insp.","NO2 WBP discharge valve BA515 2 way valve in use instead of 3 way valve in CCR console.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.1","Very High","","","RO raised for new 3 way valve. Switch renewed","2021-11-21T23:59:35","DBAU210160","Completed","2021-11-18T23:59:35","No","No","No","Internal"]
[null,null,null,20295,null,"24_15/07/2021 3:37:44 PM","2021-06-23T23:59:35","Defect","Ship Staff","Ship Staff Insp.","5P WBT stripper valve temporary switch installed on ccr cosnole.Correct switch to be instaled.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.1","Very High","","","RO raised for valve switch. Switch already renewed","2021-11-21T23:59:35","DBAU210160","Completed","2021-11-18T23:59:35","No","No","No","Internal"]
[null,null,null,20296,null,"24_14/7/2021 5:19:14 PM","2021-06-25T23:59:35","Observation","Ship Staff","Nav Audit / Verification","BNWAS panel showing error. PCB to be renewed for new battery to be detected.","Navigation - VDR / BNWAS","Navigation","Equipment Related","","","","","Upgraded PCB replaced,working satisfactorily","2021-09-24T23:59:35","DBAU215145","Completed","2021-09-26T23:59:35","No","No","No","Internal"]
[null,null,null,20304,null,"24_13/7/2021 9:52:00 PM","2021-07-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","1 NO gmdss radio not operational.","Navigation - GMDSS & Communication","Communication","Equipment Related","4.21","High","","","troubleshooting to be carried out.Loose wire connection found.Radio operational.","2021-07-22T23:59:35","","Completed","2021-07-06T23:59:35","No","No","No","Internal"]
[null,null,null,20297,null,"24_16/07/2021 7:47:40 AM","2021-07-06T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Slight grooving observed on stbd side no 2 fairlead and poop deck aft port side fairlead.","Deck - Mooring Machinery","Mooring","Equipment Related","9.1","Low","","","Build up work to be carried out.\nGrooves temporary built up.  Final built up to be carried out at Next due  Dry dock. Dry dock specs raised in REFMAN.","2022-02-19T23:59:35","","Completed","2022-11-24T23:59:35","No","No","No","Internal","Please update the job status."]
[null,null,null,20300,null,"24_16/07/2021 7:50:42 AM","2021-07-06T23:59:35","Defect","Ship Staff","Suptd. Insp.","Few of the hydraulic lines for forward windlass port and stbd are rusted.","Deck - Machinery","Mooring","Equipment Related","9.1","Low","","","Rusted sections De rusted, buffed and Painted","2022-02-19T23:59:35","","Completed","2021-08-01T23:59:35","No","No","No","Internal"]
[null,null,null,20298,null,"24_24/07/2021 6:01:30 AM","2021-07-15T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Exhaust gas boiler outlet exhaut bellow damaged","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","",""," There is no visible leakage, spare onboard","2021-10-14T23:59:35","","Completed","2021-10-11T23:59:35","No","No","No","Internal"]
[null,null,null,20301,null,"24_24/07/2021 5:56:55 AM","2021-07-15T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Stern tube fwd seal clamp ring damaged","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","clamp ring renewed in drydock by yard.","2024-01-30T23:59:35","","Completed","2024-02-28T23:59:35","No","No","No","Internal",""]
[null,null,null,20483,null,"24_16/08/2021 3:00:22 PM","2021-07-23T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Elevator not operational","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","Elevator technician attended at Singapore, he changed the parts, now elevator is operational","2021-11-21T23:59:35","","Completed","2021-10-04T23:59:35","No","No","No","Internal"]
[null,null,null,20484,null,"24_12/08/2021 12:32:18 AM","2021-08-02T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Acetylene and Oxygen hoses are connected by jubilee clips.Hoses shoukld be connected by ear clamps,using pincer tool.","Miscellaneous","Safety / LSA / FFA","Equipment Related","5.26","Medium","","","Jubilee clips replaced by ear clips","2021-11-21T23:59:35","","Completed","2021-10-07T23:59:35","No","No","No","Internal"]
[null,null,null,21075,null,"24_19/09/2021 2:06:30 PM","2021-08-25T23:59:35","Critical Equipment","Owner / Marine / Tech. Suptd.","Suptd. Insp.","135 LTRS Trolley Foam Extinguisher hose  renewal","LSA / FFA","Eng. / Strg. Comp.","Equipment Related","5.35","Medium","","","Hose was replaced by new one","2022-02-19T23:59:35","DBAU210212","Completed","2022-01-02T23:59:35","No","No","No","Internal","spare  already supplied  on 22 nd nov 2021. why is the job still pending?"]
[null,null,null,21076,null,"24_20/09/2021 2:24:48 PM","2021-08-28T23:59:35","Critical Equipment","Ship Staff","Ship Staff Insp.","Fixed Gas Detection System for Pump Room is malfunctioning ","Miscellaneous","Cargo / Ballast Systems","Equipment Related","8.1","Very High","",""," O2 Sensor replaced by new one","2021-10-22T23:59:35","","Completed","2021-09-24T23:59:35","No","No","No","Internal"]
[null,null,null,21752,null,"24_16/10/2021 3:17:09 PM","2021-09-14T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","Atmospheric condenser sea water inlet and outlet pipe  corroded & rusted, leaking from two section","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.31","Very High","","","Atm condenser S.W. outlet pipes ( 2pcs) new fabricated and damaged pipes were replaced with new fabricated pipes.","2021-12-13T23:59:35","","Completed","2021-12-02T23:59:35","No","No","No","Internal"]
[null,null,null,21760,null,"24_22/10/2021 5:42:26 PM","2021-10-04T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ER blower casing Port fwd unit’s mist catcher plates observed shifted ","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","11.8","Low","","","To regulary check and keep the mist catcher plates aligned, to be done at DD.","2022-02-19T23:59:35","","Completed","2022-07-24T23:59:35","No","No","No","Internal"]
[null,null,null,21761,null,"24_22/10/2021 7:15:09 PM","2021-10-04T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Funnel deck - Old drums kept on funnel deck – spolining the deck with rust weepings","Miscellaneous","General Appearance","Behaviour Based","11.8","Low","","","Empty old drums were cut and to be to discard ashore. Some drums transfer to C deck. ","2021-12-21T23:59:35","","Completed","2021-10-17T23:59:35","No","No","No","Internal"]
[null,null,null,21762,null,"24_22/10/2021 7:17:53 PM","2021-10-04T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Funnel casing - Fwd side /china passage side dirty","Miscellaneous","General Appearance","External Factors","11.8","Low","","","Wash with Oxalic acid ","2022-02-19T23:59:35","","Completed","2022-01-01T23:59:35","No","No","No","Internal"]
[null,null,null,21763,null,"24_22/10/2021 7:22:28 PM","2021-10-04T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Provision cranes - Both crane’s oil level gauge glass dirty – not clear","Deck - Machinery","General Appearance","Equipment Related","8.73","Medium","",""," Prov. Crane (P)  oil renwed and gauge glass cleaned, Prov Crane (S)  gauge glass cleaned, now level is visible.","2021-12-22T23:59:35","","Completed","2021-12-04T23:59:35","No","No","No","Internal"]
[null,null,null,21764,null,"24_21/10/2021 10:51:20 PM","2021-10-04T23:59:35","Critical Equipment","Owner / Marine / Tech. Suptd.","Suptd. Insp.","#2 Steering Gear motor was running-observed abnormal noise from motor unit","Critical Equip.","Eng. / Strg. Comp.","Equipment Related","10.39","High","","","S/G Motor#1&2 started one by one and S/G tested with each motor at anchorage. No abnormal noise observed.  \n\n\n\n","2021-12-22T23:59:35","","Completed","2021-12-05T23:59:35","No","No","No","Internal"]
[null,null,null,21765,null,"24_22/10/2021 9:35:40 AM","2021-10-04T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Threre are various hoses stored in Steering Gear &  Common Deck Store","Deck - Pipe / Fittings","Eng. / Strg. Comp.","Behaviour Based","","","",""," All hoses sorted out and marked with hose number and crane name and stored properly.","2021-11-21T23:59:35","","Completed","2021-11-13T23:59:35","No","No","No","Internal"]
[null,null,null,21766,null,"24_22/10/2021 7:32:10 PM","2021-10-04T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Mooring winches - Brake indicators (set point) not matching with present locked/applied condition","Deck - Mooring Machinery","Mooring","Equipment Related","9.15","Medium","",""," Defect rectified","2021-12-21T23:59:35","","Completed","2021-10-11T23:59:35","No","No","No","Internal"]
[null,null,null,21767,null,"24_22/10/2021 7:34:58 PM","2021-10-04T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Deck seal -  Float switch conduit pipe undersides rusted","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.27","Medium","","","To derust and coat – else will get holed and water may enter the conduit pipes","2021-12-22T23:59:35","","Completed","2021-12-11T23:59:35","No","No","No","Internal"]
[null,null,null,21768,null,"24_22/10/2021 7:38:06 PM","2021-10-04T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Steel plates on main deck - All newly replaced steel plates on main deck, has the welded joints rusted in its seams","Deck - Pipe / Fittings","General Appearance","Behaviour Based","11.6","Medium","","","To properly derust, apply primer and then coat","2021-11-04T23:59:35","","Completed","2021-11-04T23:59:35","No","No","No","Internal"]
[null,null,null,21769,null,"24_22/10/2021 7:40:17 PM","2021-10-04T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Pipe stacks - Rust weep marks were observed below pipe stacks on deck","Deck - Pipe / Fittings","General Appearance","Behaviour Based","11.3","Medium","","","Understand weekly HP wash of main deck and outfittings are not being followed up – to carry of hydro blasting on the weep marks and aplly coat and ensure regular HP wash (at 100 bar) is carried out every week diligently fwd to aft\nMain deck rust week mark below pipe line completed. Continious spot hydroblasting near main deck cross over continuing.\n","2022-02-19T23:59:35","","Completed","2022-09-23T23:59:35","No","No","No","Internal"]
[null,null,null,21770,null,"24_22/10/2021 7:43:04 PM","2021-10-04T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Gangway\tAngle indicators paint faded/dirty","Deck - Machinery","General Appearance","Equipment Related","5.47","Medium","","","Buffed, Painted and new marking made","2021-10-19T23:59:35","","Completed","2021-10-09T23:59:35","No","No","No","Internal"]
[null,null,null,21771,null,"24_22/10/2021 7:45:43 PM","2021-10-04T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Main deck - Area below all foam monitors have sever rust weep marks","Deck - Pipe / Fittings","General Appearance","Behaviour Based","11.3","Medium","","","First to arrest any leaks from Foam monitors and take up derusting/coating below these locations.\n\nAll leaks from Foam monitor checked and arrested.  Rust weep marks cleaned and Painted final coat green on deck.","2022-02-19T23:59:35","","Completed","2022-09-19T23:59:35","No","No","No","Internal"]
[null,null,null,21772,null,"24_22/10/2021 7:47:55 PM","2021-10-04T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Mid ship light mast - Conduit pipes in light mast rusted","Deck - Pipe / Fittings","General Appearance","Behaviour Based","11.5","Medium","","","To take up maintenance","2021-12-22T23:59:35","","Completed","2021-12-02T23:59:35","No","No","No","Internal"]
[null,null,null,21773,null,"24_22/10/2021 7:50:14 PM","2021-10-04T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Cross decks - Conduit pipe supports (running crossdeck) for Tank level gauging pipes/cabes – support brackets are rusted, spoiling the deck","Deck - Pipe / Fittings","General Appearance","Behaviour Based","11.5","Medium","",""," Rust removed and painted.","2022-02-19T23:59:35","","Completed","2022-08-20T23:59:35","No","No","No","Internal"]
[null,null,null,21774,null,"24_22/10/2021 7:51:53 PM","2021-10-04T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Fwd Bosun store - Ceiling has scattered fungus and dark patches","Miscellaneous","General Appearance","Behaviour Based","11.12","Low","","","To wash the complete ceiling during long voyage .\ncleaned  and job completed.","2022-02-19T23:59:35","","Completed","2022-08-03T23:59:35","No","No","No","Internal","Please take this job up as it is long pending."]
[null,null,null,21775,null,"24_22/10/2021 7:53:28 PM","2021-10-04T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Accomm block - Scattered spot rusts at various locations","Accommodation","General Appearance","Behaviour Based","11.8","Low","","","Spot derusting on main deck completed.  \nContionus job with hydroblaster on weather deck will be contiuned. ","2022-02-19T23:59:35","","Completed","2022-09-23T23:59:35","No","No","No","Internal","Long pending job should be taken up on urgent basis."]
[null,null,null,21776,null,"24_21/10/2021 10:32:41 PM","2021-10-04T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ER Bell Book Singapore arrival events not recorded","Miscellaneous","Cert. & Docu.","Behaviour Based,Human Error","","","","","To ensure documentation part is done correctly and timely","2021-10-04T23:59:35","","Completed","2021-10-04T23:59:35","No","No","No","Internal"]
[null,null,null,21777,null,"24_22/10/2021 3:36:22 PM","2021-10-04T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Hygrometer, wet bulb temp container empty (no water)","Navigation - Others","Navigation","External Factors,Human Error","4.7","High","","","Wet bulb container filled with water immediately. All OOW instructed to check during every watch and refill as required.","2021-10-04T23:59:35","","Completed","2021-10-04T23:59:35","No","No","No","Internal"]
[null,null,null,21778,null,"24_22/10/2021 5:20:21 PM","2021-10-04T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Aux engines all 3 Oilmax centrifugal filter was found not in use","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.9","Medium","","","To put in use immediately and ensure all 3 pumps are kept running continuously – While Engine is running/in use and whilst Engine is stopped as well.","2021-10-04T23:59:35","","Completed","2021-10-04T23:59:35","No","No","No","Internal"]
[null,null,null,21779,null,"24_22/10/2021 5:29:50 PM","2021-10-04T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ER blower spare impeller looks dirty","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Impeller cleaned and a coat of paint applied.","2021-10-19T23:59:35","","Completed","2021-10-13T23:59:35","No","No","No","Internal"]
[null,null,null,21780,null,"24_22/10/2021 5:33:05 PM","2021-10-04T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Incinerator Flue gas fan – shaft beraing grease pin was dry to sign of greased ever","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Greasing was carried out","2021-10-04T23:59:35","","Completed","2021-10-12T23:59:35","No","No","No","Internal"]
[null,null,null,21781,null,"24_22/10/2021 5:37:51 PM","2021-10-04T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","EGCS Sealing air fan motor and fan casing rusted","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.11","Medium","","","Cleaned and  a coat of paint applied.","2021-10-25T23:59:35","","Completed","2021-10-13T23:59:35","No","No","No","Internal"]
[null,null,null,21782,null,"24_21/10/2021 5:28:09 PM","2021-10-04T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","AE Spares T/C cartridge Not stowed properly in spares room – lying without proper stand in wooden box , will end up damaging the blades ","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","AE spare turbocharger was packed properly in wooden box and secured.","2021-10-12T23:59:35","","Completed","2021-10-12T23:59:35","No","No","No","Internal"]
[null,null,null,21783,null,"24_22/10/2021 7:12:08 PM","2021-10-04T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","AUS vacuum pump - Vacuum pump motor space (near ER officers change room) floor dirty with oil","Cargo Mach.","Cargo / Ballast Systems","Behaviour Based","6.4","High","","","Vacuum pump motor room floor cleaned properly.","2021-10-12T23:59:35","","Completed","2021-10-12T23:59:35","No","No","No","Internal"]
[null,null,null,21784,null,"24_22/10/2021 5:40:30 PM","2021-10-04T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","EGCS Top bracing stay bolts are getting rusted","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.11","Medium","","","To either regularly grease or apply paint to avoid corrossion- cleaned and grease applied.","2021-10-19T23:59:35","","Completed","2021-10-13T23:59:35","No","No","No","Internal"]
[null,null,null,21785,null,"24_22/10/2021 7:26:37 PM","2021-10-04T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Mooring winches - All Mooring winches brake band stopper bolts – clearance haywire","Deck - Mooring Machinery","Mooring","Equipment Related","9.1","Low","","","All Mooring winches brake band support  bolts clearance checked and adjusted as per manual. ","2021-10-19T23:59:35","","Completed","2021-10-13T23:59:35","No","No","No","Internal"]
[null,null,null,21786,null,"24_22/10/2021 7:29:31 PM","2021-10-04T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Hydro blaster - Reported not operational","Deck - Machinery","General Appearance","Equipment Related","","","","","Hydro blaster repaired and is working satisfactorily.","2021-10-09T23:59:35","","Completed","2021-10-09T23:59:35","No","No","No","Internal"]
[null,null,null,21787,null,"24_22/10/2021 7:03:54 PM","2021-10-04T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Safety stores in upper deck. Items lying haphazardly","LSA / FFA","General Appearance","Behaviour Based","11.13","Low","","","SAFETY STORE ARRANGED PROPERLY. ALL ITEMS IN PLACE AND SECURED.","2021-11-03T23:59:35","","Completed","2021-10-06T23:59:35","No","No","No","Internal"]
[null,null,null,21753,null,"24_21/10/2021 5:24:26 PM","2021-10-04T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ECR AC Unit Pressure gauges defective - #1 Suc press gauge, #2 HP press gauge","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Renewed after collecting all the gases and recharged the system.","2022-02-19T23:59:35","","Completed","2022-08-25T23:59:35","No","No","No","Internal","-\tIs spare available on board. Please raise RO for new gauges if not raised/received."]
[null,null,null,21754,null,"24_21/10/2021 5:41:45 PM","2021-10-04T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Spares storage space Electrical various consumable stores items lying loose and haphazardly ","Miscellaneous","General Appearance","Equipment Related","","","",""," Electrical consumables in stores arranged and secured","2021-10-19T23:59:35","","Completed","2021-10-16T23:59:35","No","No","No","Internal"]
[null,null,null,21755,null,"24_21/10/2021 10:24:57 PM","2021-10-04T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Accommo. AC unit touch screen panel faded","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","Presently working satisfactorily. Spares onboard can be done when the vessel trading at Low temperature areas.","2022-03-22T23:59:35","DBAU210243","Completed","2022-09-17T23:59:35","No","No","No","Internal","Spare screen has been supplied. Please update if same has been installed or not."]
[null,null,null,21756,null,"24_21/10/2021 10:44:07 PM","2021-10-04T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Aux Boilers remote release levers for gauge cocks, valves -seized and few got stuck in one position","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","Aux. boiler remote release levers for gauge glass made free and greased. Now operating properly.","2021-11-21T23:59:35","","Completed","2021-11-09T23:59:35","No","No","No","Internal"]
[null,null,null,21757,null,"24_22/10/2021 5:18:08 PM","2021-10-04T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Cascade tank Steam controller for the heating steam to tank – continuous leaking from valve top","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Leakage rectified","2021-10-19T23:59:35","","Completed","2021-10-21T23:59:35","No","No","No","Internal"]
[null,null,null,21758,null,"24_22/10/2021 5:24:57 PM","2021-10-04T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ME L.O.water sensor Observed display showing 0.448 – but no alarm in display","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","",""," As per instruction manaul value within limit.","2021-10-05T23:59:35","","Completed","2021-10-05T23:59:35","No","No","No","Internal"]
[null,null,null,21759,null,"24_22/10/2021 5:26:49 PM","2021-10-04T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Ac cooling units supplied for Boiler and DPU  panels not yet installed","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.11","Medium","","","Air conditioner fitted in place and tried out found working satisfactorily.","2022-03-22T23:59:35","","Completed","2022-12-28T23:59:35","No","No","No","Internal","Job is overdue.  Share plan for installation."]
[null,null,null,20299,null,"24_24/07/2021 6:07:22 AM","2021-10-15T23:59:35","Observation","Ship Staff","Ship Staff Insp.","No.3 Cooling sea water pump mechanical seal leak","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Pump opend found shaft thread for locking nut  damaged, RO raised for new shaft. New shaft received & installed. tried out pump & in order.","2022-03-22T23:59:35","DBAU210241","Completed","2022-03-07T23:59:35","No","No","No","Internal","Spares are ready, will be supplied to vsl."]
[null,null,null,22688,null,"24_22/11/2021 12:37:34 AM","2021-10-26T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Fwd fire wire reel reducer motor shaft & bearing broken.","Deck - Mooring Machinery","Mooring","Equipment Related","","","","","To renew or fabricate new fire wire reel reducer motor shaft & renew bearing . Reducer motor  was landed for repair. Recieved reconditionedreducer motor. fixed back and tested.","2022-01-21T23:59:35","","Completed","2022-01-11T23:59:35","No","No","No","Internal"]
[null,null,null,22689,null,"24_22/11/2021 12:29:14 AM","2021-10-30T23:59:35","Defect","Ship Staff","Ship Staff Insp.","4P WBT sounding pipe broken under the main deck.","Hull & Tanks","Cargo / Ballast Systems","Equipment Related","","","","","4P WBT sounding pipe temporary repaired by putting rubber hose and secured it by cable ties.","2021-11-01T23:59:35","","Completed","2021-11-01T23:59:35","No","No","No","Internal"]
[null,null,null,22717,null,"24_30/11/2021 4:20:04 AM","2021-11-14T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","U clamp of few hydraulic lines are completely corroded.","Deck - Pipe / Fittings","General Appearance","Equipment Related","","","","","Corroded U clamp of hydraulic lines De rusted/Buffed and Painted","2022-03-22T23:59:35","","Completed","2022-05-18T23:59:35","No","No","No","Internal"]
[null,null,null,22718,22718,"24_30/11/2021 4:32:22 AM","2021-11-14T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Various shelter on deck are in rusted condition","Miscellaneous","General Appearance","Equipment Related","5.38","High","","","Shelter were derusted, buffed and painted.","2022-03-22T23:59:35","","Completed","2022-01-25T23:59:35","No","No","No","Internal"]
[null,null,null,22719,null,"24_30/11/2021 4:45:16 AM","2021-11-14T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","EGCS room louvers in rusted condition. To be derusted and paint.","Miscellaneous","General Appearance","Equipment Related","","","","","cleaned and painted.","2022-02-19T23:59:35","","Completed","2022-09-05T23:59:35","No","No","No","Internal"]
[null,null,null,22720,null,"24_30/11/2021 4:49:34 AM","2021-11-14T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Emergency DG DO tank vent head & save all in rusted condition.","Deck - Pipe / Fittings","General Appearance","Equipment Related","","","","","Derusted, buffed and painted","2022-02-19T23:59:35","","Completed","2022-01-28T23:59:35","No","No","No","Internal"]
[null,null,null,22722,null,"24_30/11/2021 11:37:15 AM","2021-11-14T23:59:35","Observation","Others (Eg. Insurance etc.)","Others (Eg. Insurance etc.)","Atmospheric condenser SW outlet pipe has leakage sign. To clean and rectify if required.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","There is no leak from sea water pipe, old marks were there, same were cleaned and painted.","2021-11-23T23:59:35","","Completed","2021-11-17T23:59:35","No","No","No","External"]
[null,null,null,22723,null,"24_30/11/2021 11:43:12 AM","2021-11-14T23:59:35","Observation","Others (Eg. Insurance etc.)","Others (Eg. Insurance etc.)","All weather tight doors of EGCs room are not marked with open / close marking for its dog handle","Miscellaneous","General Appearance","Equipment Related","","","","","Open/Close markings stencilled on EGCS weather tight doors.","2021-11-21T23:59:35","","Completed","2021-11-17T23:59:35","No","No","No","External"]
[null,null,null,22724,null,"24_30/11/2021 11:46:55 AM","2021-11-14T23:59:35","Observation","Others (Eg. Insurance etc.)","Others (Eg. Insurance etc.)","The stored pipes in engine room to be secured by wire lashing.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Behaviour Based","","","","","Stored pipes were secured by waire lashing","2021-11-23T23:59:35","","Completed","2021-11-18T23:59:35","No","No","No","External"]
[null,null,null,22725,null,"24_30/11/2021 4:28:16 AM","2021-11-14T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","None of the level gauge of winch & windlass are clear to check the oil level. Plan to clean or renew as required","Deck - Mooring Machinery","Mooring","Equipment Related","","","","","All winches & windlass oil level gauge were cleaned. Some level gauge with paint were removed .","2022-01-01T23:59:35","","Completed","2021-11-18T23:59:35","No","No","No","Internal"]
[null,null,null,22726,null,"24_30/11/2021 11:51:10 AM","2021-11-14T23:59:35","Observation","Others (Eg. Insurance etc.)","Others (Eg. Insurance etc.)","Engine room spare part room need to arrange","Miscellaneous","General Appearance","Human Error","","","","","Engine room store was arranged properly.","2021-11-23T23:59:35","","Completed","2021-12-20T23:59:35","No","No","No","External"]
[null,null,null,22727,null,"24_30/11/2021 4:38:07 AM","2021-11-14T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Water collected below the ballast pump in pump room . To check for leakage and pumproom to maintain in water free condition.","Cargo Mach.","General Appearance","Equipment Related","","","","","Water collected below ballast pump in the pump room  were cleaned & dried","2021-12-06T23:59:35","","Completed","2021-11-20T23:59:35","No","No","No","Internal"]
[null,null,null,23158,null,"24_18/12/2021 12:52:35 PM","2021-11-16T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Oil leak from ME L.O. pump no.1 oil seal","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","ME L.O. pump no.1 oil seal replaced with new spare oil seal, now pump is working satisfactory without any leak.","2022-02-15T23:59:35","","Completed","2021-11-29T23:59:35","No","No","No","Internal"]
[null,null,null,22721,null,"24_30/11/2021 1:57:16 PM","2021-11-17T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Forward  Electric Whistle piston & piston ring broken","Navigation - Others","Navigation","Equipment Related","","","","","Piston, piston ring, cylinder and con rod   renewed and tried out, working satisfactorily.","2022-01-22T23:59:35","DBAU210280","Completed","2022-01-11T23:59:35","No","No","No","Internal"]
[null,null,null,23160,null,"24_17/12/2021 8:13:28 AM","2021-11-28T23:59:35","Defect","Ship Staff","Ship Staff Insp.","MW06 Hydraulic  return line corroded and found pit hole.","Deck - Pipe / Fittings","Mooring","Equipment Related","","","","","MW06 hydraulic return line was disconnected. New line was fabricated.And will fix back when completed","2021-12-09T23:59:35","","Completed","2021-12-09T23:59:35","No","No","No","Internal"]
[null,null,null,23157,null,"24_12/12/2021 4:05:13 AM","2021-12-03T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Corroded light bulb base pipe on radar mast","Navigation - Others","Navigation","Equipment Related","4.8","Medium","","","Repairs on the X-mas light completed.","2022-12-10T23:59:35","","Completed","2022-11-18T23:59:35","Yes","No","No","Internal","Share recent photograph of the light base. Inspection of the X-mas lights also to be carried out and share if you find any more defects and damages."]
[null,null,null,23159,null,"24_17/12/2021 8:24:45 AM","2021-12-04T23:59:35","Defect","Ship Staff","Ship Staff Insp.","While derusting Slop P heating coil steam line pipe, hole were  found corroded on the part.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","","","","","Steam line pipe were discconected and were brought to engine work shop. Hot work were carried out on the pipe. ","2021-12-11T23:59:35","","Completed","2021-12-09T23:59:35","No","No","No","Internal"]
[null,null,null,23734,null,"24_20/01/2022 11:34:48 AM","2021-12-23T23:59:35","Defect","Ship Staff","Ship Staff Insp.","L.T. Cooler (FWD) S.W. inlet valve flap stuck in partial open position, valve spindle is free.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.31","Very High","","","L.T. Cooler S.W. inlet valve replaced by new one.","2022-02-19T23:59:35","DBAU220002","Completed","2022-01-15T23:59:35","No","No","No","Internal","spare are ready and will be connected to vls soon."]
[null,null,null,23735,null,"24_21/01/2022 6:34:10 AM","2021-12-23T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Windlass Motor (STBD) FWD Pressure Block body rusted/corroded,minor oil sippage observed","Deck - Mooring Machinery","Mooring","Equipment Related","","","",""," Pressure Block replaced by one and windlass tried out,found working satisfactorily.","2022-02-19T23:59:35","","Completed","2022-01-22T23:59:35","No","No","No","Internal"]
[null,null,null,24070,null,"24_27/02/2022 12:34:07 PM","2022-01-07T23:59:35","Observation","Ship Staff","Ship Staff Insp.","IG Scrubber Tower water sippage found from bottom plate. Bottom plate checked found pitted at various places.","Inert Gas","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Presently no leaks noted and holding good. Reported the same in REFMAN to be done in next DD.","2022-03-22T23:59:35","","Completed",null,"No","No","No","Internal","Is there any leakage at present. If not then this job to be reported in REFMAN and defect to closed out in DDRL."]
[null,null,null,23993,null,"24_07/02/2022 4:10:57 PM","2022-01-17T23:59:35","Defect","Ship Staff","Ship Staff Insp.","L.T. Cooler (FWD) sea water outlet valve found stuck in close position","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","",""," L.T.Cooler (FWD)  sea water outlet valve  replaced by new one.","2022-01-27T23:59:35","","Completed","2022-01-19T23:59:35","No","No","No","Internal"]
[null,null,null,24074,null,"24_28/02/2022 3:38:25 AM","2022-01-25T23:59:35","Defect","Ship Staff","Ship Staff Insp.","A pin hole leak found on hydraulic return line of hydraulic box no. 4A","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","Hydraulic return line line was disconnected. brought to engine work shop for hotwork repair. Painted and installed back and tested.","2022-01-26T23:59:35","","Completed","2022-01-26T23:59:35","No","No","No","Internal"]
[null,null,null,24073,null,"24_28/02/2022 3:47:51 AM","2022-02-05T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Gangwaylashing  securing arrangement found corroded","Deck - Pipe / Fittings,Miscellaneous","Safety / LSA / FFA","Equipment Related","","","","","Fabricated gangway lashing  securing arrangement","2022-02-07T23:59:35","","Completed","2022-02-07T23:59:35","No","No","No","Internal"]
[null,null,null,24071,null,"24_27/02/2022 12:21:55 PM","2022-02-15T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Main Engine Air Cooler (Aft)  found air leakage from end cover","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Renewed O-ring and tried out found no leaks.","2022-03-22T23:59:35","","Completed","2022-09-30T23:59:35","No","No","No","Internal"]
[null,null,null,24072,null,"24_27/02/2022 12:45:27 PM","2022-02-17T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Acco. A/C Compressor No.1&2 pressure  sensors terminal box wiring cables/connectors are in very bad condition. Wirings are shorting and giving false alarm/irratic output.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","11.11","Very High","","","Fault cables renewed and secured.","2022-03-22T23:59:35","","Completed","2022-06-24T23:59:35","No","No","No","Internal"]
[null,null,null,24463,null,"24_16/03/2022 2:06:09 PM","2022-02-25T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Elevator Door not opening on E1 Deck.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","Door safety switch magnet found defective. renewed with new received spare. In order.","2022-05-28T23:59:35","DBAU220047","Completed","2022-04-16T23:59:35","No","No","No","Internal"]
[null,null,null,24464,null,"24_16/03/2022 5:14:53 PM","2022-02-25T23:59:35","Observation","Ship Staff","Ship Staff Insp.","EGCS SW Ovbd Line Discharge Valve (Fwd) stuck in 'Open' Position.","E/R - Main Engine,E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Renewed the valve","2022-11-27T23:59:35","","Completed","2022-11-09T23:59:35","No","No","No","Internal","Shore team attended the vessel to renew the valve in Singapore in August but job couldn't be completed due to external factors. we will plan this job during proper anchorage as we need to plug the overboard line. Target date to be extended."]
[null,null,null,24465,null,"24_16/03/2022 5:18:04 PM","2022-02-25T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Scrubber GRE outlet pipe, connectors for sensor fittings, need to check all for corrosion and preventive measures to be taken.","E/R - Main Engine,E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Inspected and renewed as necessary.","2022-05-28T23:59:35","","Completed","2022-09-10T23:59:35","No","No","No","Internal","Please update the status. Job should have been completed by now."]
[null,null,null,24466,null,"24_16/03/2022 5:29:30 PM","2022-02-25T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ECR door latch damaged","Accommodation,Miscellaneous","Safety / LSA / FFA","Equipment Related","","","","","ECR door latch to be rectified. All Door latches checked & found damaged at various locations. Rectified & in use.","2022-05-28T23:59:35","NA","Completed","2022-04-03T23:59:35","No","No","No","Internal"]
[null,null,null,24467,null,"24_16/03/2022 5:31:25 PM","2022-02-25T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Lub Oil IBCs on port side C deck to transfer to respective tanks.","Miscellaneous","General Appearance","Equipment Related","11.3","Medium","","","Transfered all to AE Lub oil Settling tank.","2022-05-28T23:59:35","","Completed","2022-12-06T23:59:35","No","No","No","Internal","This defect found still open???"]
[null,null,null,24468,null,"24_16/3/2022 8:41:05 PM","2022-02-25T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Cargo  &  Ballast valves not operating satisfactorily.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.11","Medium","","","CL235,CL236,CL247,CL206 and BA 416 Value need to Operated from Deck Local stands. CL241, CL157,CL126 and CL124 , BA407, BA409,CL 231 CL232,CL128, CL 244 Open / Close Indication Not working from CCR. Valve Indicators & solenoid blocks renewed. Following valves still not operating properly. Indicators for CL 241, CL 157, CL 128, CL 244, CL 231, CL 232 & Valve operation for CL206,CL236, BA416.\nAll valves except BA 416 , CL206 and CL236 need to opened locally others operating from CCR.  Awaiting spares to repair for  above 3 vlaves","2022-05-28T23:59:35","RO  DBAU220016","Completed","2022-09-23T23:59:35","No","No","No","Internal","Please update the status of the valves."]
[null,null,null,24469,null,"24_03/16/2022 2:49:31 PM","2022-02-25T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Elevator various buttons in Cage & in Accomodation not working or holder damaged.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Presently working satisfactorily.","2022-05-28T23:59:35","DBAU220047","Completed","2022-08-27T23:59:35","No","No","No","Internal","Spares as per DBAU220047 were supplied in April 2022. One more order was raised and that also supplied. Please update the status."]
[null,null,null,24470,null,"24_18/03/2022 1:42:01 PM","2022-02-25T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","EGB Inspection Doors Exhaust Gas Leak.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","Gaskets of doors renewed.","2022-05-28T23:59:35","NA","Completed","2022-03-19T23:59:35","No","No","No","Internal"]
[null,null,null,24471,null,"24_19/03/2022 2:20:29 PM","2022-02-25T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Galley entrance door tied with ropes.","Accommodation","General Appearance","Inappropriate Procedure","11.13","Low","","","Proper securing arrangement fabricated.","2022-03-28T23:59:35","","Completed","2022-02-25T23:59:35","No","No","No","Internal"]
[null,null,null,24472,null,"24_19/03/2022 2:43:35 PM","2022-02-25T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Derusting & renewal of manifold grating ","Deck - Pipe / Fittings","General Appearance","External Factors","","","","","Old rusted/wasted gratings  replaced with the new supplied gratings.","2022-05-28T23:59:35","","Completed","2022-04-09T23:59:35","No","No","No","Internal"]
[null,null,null,24473,null,"24_19/03/2022 2:49:14 PM","2022-02-25T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Brake band metal top plate for fire wire securing drum fwd area is wasted.","Deck - Mooring Machinery","Mooring","Equipment Related","9.15","Medium","","","Fire wire storage drum and Brake band drum assembly fabricated and fitted in position.","2023-04-23T23:59:35","","Completed","2023-04-20T23:59:35","No","No","No","Internal","Way past due date. Status update?"]
[null,null,null,24474,null,"24_16/03/2022 5:52:54 PM","2022-02-25T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Cleaning and painting of engine room workshop.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Cleaned, painted soap washed the bulkheads.","2022-05-28T23:59:35","","Completed","2022-08-16T23:59:35","No","No","No","Internal"]
[null,null,null,24475,null,"24_19/03/2022 2:37:00 PM","2022-02-25T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Support bracket for VRCS hydraulic line are corroded.","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","Equipment Related","8.11","Medium","","","Maintenance for the  support bracket for the VRCS hydraulic line carried out.  2 Sections of VRCS line renewed. ","2022-05-28T23:59:35","","Completed","2022-09-23T23:59:35","No","No","No","Internal"]
[null,null,null,24476,null,"24_19/03/2022 2:54:08 PM","2022-02-25T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Wheels for various valves on deck are wasted.","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","Equipment Related","5.38","High","","","Matainance for wheels for various valves on deck to be carried out & to be replaced with the new wheels.\nAll other valves are rectified, only air line valve needs to be rectified\nAll Broken wheels on deck renewed.","2022-02-25T23:59:35","","Completed","2022-09-23T23:59:35","No","No","No","Internal"]
[null,null,null,24477,null,"24_19/03/2022 2:58:22 PM","2022-02-25T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Foam monitor direction spring are wasted .","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.35","Medium","","","Foam monitor direction spring removed & cleaned/wire brushed. Thin coating of silver paint applied on all springs & installed back. Same tried out & found operating satisfactorily. No need for renewal of springs. The RO DBAU220007 can be cancelled.","2022-03-28T23:59:35","DBAU220007","Completed","2022-05-23T23:59:35","No","No","No","Internal"]
[null,null,null,24480,null,"24_19/03/2022 2:28:50 PM","2022-02-25T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Wheel broken for the valve on the separator unit on yellow line inside  pumproom","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","New wheel for the valve on the separator unit replaced.","2022-04-27T23:59:35","","Completed","2022-03-11T23:59:35","No","No","No","Internal"]
[null,null,null,24502,null,"24_16/03/2022 5:50:41 PM","2022-02-25T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Oil in Engine room on Port side bulkhead.\t","E/R - Aux. Engine,E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","AE #3 DO LIne Outlet valve bonnet found leaking. Valve bonnet gasket renewed & leak rectified. In order.","2022-05-28T23:59:35","","Completed","2022-02-25T23:59:35","No","No","No","Internal"]
[null,null,null,24503,null,"24_16/03/2022 5:20:18 PM","2022-02-25T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Steering gear oil leaks to identify and rectify.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Steering gear pressure gauge fittings oil leaks rectified & area cleaned. In order.","2022-05-28T23:59:35","","Completed","2022-03-01T23:59:35","No","No","No","Internal"]
[null,null,null,24504,null,"24_16/03/2022 5:23:21 PM","2022-02-25T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Open grease drum in AUS motor room, oil can in emer gen room and several other locations in ER.","Accommodation,Miscellaneous","General Appearance","Human Error","","","","","Stress to be given on General Houskeeping. All areas checked & rectified oil/cans/rags.","2022-05-28T23:59:35","NA","Completed","2022-02-26T23:59:35","No","No","No","Internal"]
[null,null,null,24505,null,"24_16/03/2022 5:26:32 PM","2022-02-25T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Grey water Overboard valve on port side leaking from stem gland.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","valve stem gland nipped up & leak rectified. All other storm valves checked & found with no leaks.","2022-05-28T23:59:35","NA","Completed","2022-02-25T23:59:35","No","No","No","Internal"]
[null,null,null,24506,null,"24_16/03/2022 5:35:08 PM","2022-02-25T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ME FO/VIT racks found dry. Must be oiled on daily basis. Various ball joints on fuel governing system no grease found.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","All racks cleaned & lubricated. Duty personnel briefed on importance of keeping the racks cleaned & lubricated. All ball joints & greasing points checked. Nipples found choked at various locations. same cleared/renewed as required. Grease applied.","2022-03-11T23:59:35","NA","Completed","2022-02-27T23:59:35","No","No","No","Internal"]
[null,null,null,24478,null,"24_16/03/2022 2:00:27 PM","2022-02-26T23:59:35","Observation","Ship Staff","Ship Staff Insp.","ME Scavenge Air Differential Gauges not working.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","Gauge lines found choked. Same cleared by shipstaff during engine operation but still choked. \nSame cleared durinf stoppage. Line is clear & in use.","2022-05-29T23:59:35","NA","Completed","2022-03-20T23:59:35","No","No","No","Internal"]
[null,null,null,24479,null,"24_15/03/2022 6:49:59 PM","2022-02-26T23:59:35","Observation","Ship Staff","Ship Staff Insp.","AE#3 starting air not sufficient to start the engine.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","AE#3 Starting Air motor renewed with onboard overhauled spare. Issue not resolved. Both starting air valves & controller overhauled. Issue still not resolved. Checked AE#1 & AE#2. Found also not starting due to insufficient air. Found the Air reducing valve malfunctioning. Stby valve also not functioning. Overhauled one reducing valve. All AE's starting satisfactorily. Other reducing valve overhauled & in order. RO raised. Awaiting Spares.","2022-05-29T23:59:35","RO DBAU220056","Completed","2022-08-07T23:59:35","No","No","No","Internal"]
[null,null,null,24482,null,"24_16/03/2022 2:03:44 PM","2022-02-26T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Elevator COPT Platform Call station display not working.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Working satisfactorily","2022-04-28T23:59:35","DBAU220047","Completed","2022-08-07T23:59:35","No","No","No","Internal"]
[null,null,null,24483,null,"24_16/03/2022 2:08:44 PM","2022-02-26T23:59:35","Observation","Ship Staff","Ship Staff Insp.","ME Local Maneouvring Panel \"Sound Off\" lamp blinking.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Panel reset. Alarm has Reset Rectified.","2022-05-29T23:59:35","","Completed","2022-03-19T23:59:35","No","No","No","Internal"]
[null,null,null,24484,null,"24_18/03/2022 1:45:46 PM","2022-02-26T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Aux. Boiler #2 Gauge Glass found leaking","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","Gauge glass overhauled with new spares.","2022-05-29T23:59:35","NA","Completed","2022-03-12T23:59:35","No","No","No","Internal"]
[null,null,null,24488,null,"24_03/16/2022 2:55:25 PM","2022-02-26T23:59:35","Observation","Ship Staff","Ship Staff Insp.","ME LO Backwash Filters Hydraulic Motor rotation for one unit defective.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Hydraulic motors overhauled. RO to be raised for used spares.","2022-05-29T23:59:35","","Completed","2022-03-21T23:59:35","No","No","No","Internal"]
[null,null,null,24509,null,"24_16/03/2022 2:15:08 PM","2022-02-26T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Shipside bulkhead in ER port side found with heavy rust in some areas.","Hull & Tanks","Structural Condn. / WT integrity ","Equipment Related","","","","","These areas were wire brushed & cleaned. Found the damage to be minimal. Same painted.","2022-05-29T23:59:35","NA","Completed","2022-03-06T23:59:35","No","No","No","Internal"]
[null,null,null,24485,null,"24_16/03/2022 1:52:57 PM","2022-02-27T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Accom. AC Compressor #1 drawing high current.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Found the compressor LO pump incorrectly installed. Spare Compressor overhauled by shore & installed. Operating satisfactorily. Rectified.","2022-04-29T23:59:35","","Completed","2022-05-11T23:59:35","No","No","No","Internal"]
[null,null,null,24486,null,"24_16/03/2022 2:18:12 PM","2022-02-27T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Various LED tublight Casings found damaged in ER, Pumproom & on Deck.","Elect. Mach. & Equip.","General Appearance","Equipment Related","11.11","Very High","","","Renewed as necessary and made it operational.","2022-05-30T23:59:35","RO DBAU220062","Completed","2022-09-06T23:59:35","No","No","No","Internal","Spares have been supplied. Please update the status."]
[null,null,null,24487,null,"24_18/03/2022 1:34:04 PM","2022-02-27T23:59:35","Observation","Ship Staff","Ship Staff Insp.","EGCS MGPS not operating satisfactorily.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Amperes showing less than recommended. MGPS Anodes & filter opened up for inspection. Found anodes completely wasted. Some damage/erosion also found on the Filter Casing. RO raised & received spares on 14-Jun-2022. Anodes renewed & put in use.","2022-05-30T23:59:35","RO DBAU220044 & DBAU220109","Completed","2022-06-18T23:59:35","No","No","No","Internal",""]
[null,null,null,24489,null,"24_18/03/2022 1:49:16 PM","2022-02-27T23:59:35","Observation","Ship Staff","Ship Staff Insp.","AE #3 FO Filter Differential Pressure Faulty.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Sensor found damaged. Same renewed with new received spare. Tried out & in use.","2022-05-30T23:59:35","DBAU220030","Completed","2022-06-15T23:59:35","No","No","No","Internal"]
[null,null,null,24490,null,"24_18/03/2022 1:51:34 PM","2022-02-27T23:59:35","Observation","Ship Staff","Ship Staff Insp.","CW Expansion Tank Gauge Cock stuck in closed position.","E/R - Main Engine,E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Gauge Cock freed up & renewed gaskets. Rectified.","2022-05-30T23:59:35","NA","Completed","2022-03-19T23:59:35","No","No","No","Internal"]
[null,null,null,24491,null,"24_15/03/2022 6:44:30 PM","2022-02-27T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Engine Room Overhead Crane found tripping in High Mode during operation.","Elect. Mach. & Equip.,Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Renewed the contactor found working satisfactorily.","2022-05-30T23:59:35","","Completed","2022-09-24T23:59:35","No","No","No","Internal","Noted during recent ship visit, there were issues with crane operation. Trouble shooting to be carried out on as soon as possible. Please send us the findings."]
[null,null,null,24500,null,"24_03/16/2022 2:52:13 PM","2022-02-27T23:59:35","Observation","Ship Staff","Ship Staff Insp.","EGB Inlet & Outlet Exhaust Bellow leaking.","E/R - Boiler,E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","EGB Outlet bellow renewed with new spare on 09-May-2022. \n","2022-07-28T23:59:35","","Completed","2022-05-02T23:59:35","No","No","No","Internal","Outlet bellow has been renewed. Subject line to be changed to reflect the issue at hand. Raise a RO for new bellow. Raise this as a new defect in DDRL. Old issue can be closed out."]
[null,null,null,24492,null,"24_16/03/2022 2:12:36 PM","2022-02-28T23:59:35","Observation","Ship Staff","Ship Staff Insp.","EGCS SW Pump Main Discharge line Drain Stub Piece leaking.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Drain Stub piece found with pin hole leak. leak rectified by welding. tried out & in use.","2022-05-31T23:59:35","","Completed","2022-03-15T23:59:35","No","No","No","Internal"]
[null,null,null,24507,null,"24_16/03/2022 1:50:12 PM","2022-02-28T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Main LT Cooler #1 Backwash Valve Stuck/Jammed in Closed position.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Backwash valve renewed with new spare.","2022-05-02T23:59:35","NA","Completed","2022-03-01T23:59:35","No","No","No","Internal"]
[null,null,null,24508,null,"24_18/03/2022 1:36:19 PM","2022-03-01T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Cascade Tank Heating line Steam leak","E/R - Boiler,E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Heating Line flange gasket found damaged. Same replaced with new gasket. In order.","2022-06-01T23:59:35","NA","Completed","2022-03-09T23:59:35","No","No","No","Internal"]
[null,null,null,24493,null,"24_16/03/2022 1:40:05 PM","2022-03-03T23:59:35","Observation","Ship Staff","Ship Staff Insp.","AE Starting Air Line relief Valve leaking.","E/R - Aux. Engine,E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","No leaks observed, working satisfactorily.","2022-06-03T23:59:35","RO DBAU225016","Completed","2022-08-07T23:59:35","No","No","No","Internal"]
[null,null,null,24494,null,"24_18/03/2022 10:18:22 AM","2022-03-03T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Foam Room Exhaust Fan found corroded & not operational.","Elect. Mach. & Equip.,LSA / FFA,Miscellaneous","Safety / LSA / FFA","Equipment Related","11.10","Medium","","","Renewed and tried out working satisfactorily.","2022-06-03T23:59:35","DBAU220045","Completed","2022-09-21T23:59:35","No","No","No","Internal"]
[null,null,null,24495,null,"24_18/03/2022 10:20:01 AM","2022-03-03T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Emcy Gen Room Exhaust Fan found corroded & non operational.","Elect. Mach. & Equip.,LSA / FFA,Miscellaneous","Safety / LSA / FFA","Equipment Related","11.10","Medium","","","Renewed and tried out found working satisfactorily.","2022-06-03T23:59:35","DBAU220045","Completed","2022-09-23T23:59:35","No","No","No","Internal","Spare fan has been supplied. Please confirm if same has been installed in place."]
[null,null,null,24496,null,"24_16/03/2022 1:46:34 PM","2022-03-04T23:59:35","Observation","Ship Staff","Ship Staff Insp.","ME Unit #4 Cylinder Head Jacket Found leaking.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Jacket renewed with spare one","2022-05-04T23:59:35","DBAU220046","Completed","2022-03-08T23:59:35","No","No","No","Internal"]
[null,null,null,25391,64411,"24_Sat May 07 2022 14:00:23 GMT+0800","2022-03-05T23:59:35","Observation","Ship Staff","Ship Staff Insp.","AE #3 Attached Fuel Feed Pump found leaking into the LO Sump.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Feed pump mechanical seal renewed & pump overhauled. Installed back & found in order. AE #3 LO Sump drained, cleaned & refilled with fresh oil. ","2022-06-05T23:59:35","NA","Completed","2022-04-07T23:59:35","No","No","No","Internal"]
[null,null,null,24497,null,"24_16/03/2022 1:56:08 PM","2022-03-05T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Economiser Boiler Feed Pump #1 & #2 Circulation line to cascade tank found leaking.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Pinhole found in the Line. Temporarily repaired with cold work. Line to be repaired with welding. Tried out & no leak observed.","2022-05-05T23:59:35","NA","Completed","2022-05-31T23:59:35","No","No","No","Internal"]
[null,null,null,24501,null,"24_18/03/2022 1:44:07 PM","2022-03-05T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Aux. Boiler #2 FW Controller flange leak.","E/R - Boiler,E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Controller overhauled & gaskets renewed. tried out & found in order.","2022-06-05T23:59:35","NA","Completed","2022-03-12T23:59:35","No","No","No","Internal"]
[null,null,null,24498,null,"24_17/03/2022 7:45:19 PM","2022-03-06T23:59:35","Observation","Ship Staff","Ship Staff Insp.","ECDIS Back up battery renewal due on 26-Mar-2022.","Navigation - ECDIS","Navigation","Equipment Related","","","","","Battery renewed with new supplied spares. ECDIS tried out & in order.","2022-06-06T23:59:35","DBAU220039","Completed","2022-06-08T23:59:35","No","No","No","Internal","Spares supplied. Renew the battery and advise."]
[null,null,null,25400,93261,"24_Tue May 24 2022 21:26:40 GMT+0800","2022-03-09T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Cascade Tank Level Gauge found leaking.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Gauge removed & gaskets fabricated for rectifying the leak. New original gaskets ordered to be kept as per spare.","2022-06-17T23:59:35","RO DBAU220063","Completed","2022-04-17T23:59:35","No","No","No","Internal"]
[null,null,null,24499,null,"24_18/03/2022 1:39:46 PM","2022-03-09T23:59:35","Critical Equipment","Ship Staff","Ship Staff Insp.","Lifeboat #2 (Port) Engine not starting smoothly.","Critical Equip.,LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","Investigated and mad operational. found fuel liver struck.","2022-03-11T23:59:35","","Completed","2022-03-10T23:59:35","No","No","No","Internal"]
[null,null,null,25387,57821,"24_Sun May 29 2022 17:49:39 GMT+0800","2022-03-17T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Starboard midship crane Wire drum- Limit switch not working","Cargo Mach.,Deck - Machinery","Cargo / Ballast Systems","Equipment Related","10.32","Very High","","","stbd Crane Limit switch repaired.","2022-06-16T23:59:35","DBAU220110","Completed","2022-10-13T23:59:35","No","No","No","Internal","Awaiting spare supply due to long lead time"]
[null,null,null,25389,58500,"24_Sun May 29 2022 18:06:05 GMT+0800","2022-03-17T23:59:35","Critical Equipment","Ship Staff","Ship Staff Insp.","Slop Port Cargo oil tank high level alarm sensor not working.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","RO raised for the sensor. Same received & installed. High Level Alarm tried out & found operating satisfactorily.","2022-06-18T23:59:35","DBAU220061","Completed","2022-06-07T23:59:35","No","No","No","Internal","Spares have been supplied. Please renew."]
[null,null,null,25401,38629,"24_Tue May 24 2022 21:36:58 GMT+0800","2022-03-20T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Emcy Fire Pump Priming Unit not engaging.","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","Priming Unit overhauled with new spares. Tried out & found in order. RO raised in orde rtr to keep as per Critical spares inventory.","2022-06-20T23:59:35","RO DBAU220069","Completed",null,"No","No","No","Internal"]
[null,null,null,25402,90601,"0_Tue May 24 2022 21:39:33 GMT+0800","2022-03-23T23:59:35","Observation","Ship Staff","Ship Staff Insp.","HFO Tank #1 Stbd Heating Line Pipe Leaking.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Gasket found damaged. Same renewed.","2022-04-22T23:59:35","NA","Completed","2022-03-23T23:59:35","No","No","No","Internal"]
[null,null,null,25403,52586,"24_Tue May 24 2022 21:44:42 GMT+0800","2022-03-24T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Atmospheric Condenser SW outlet Line found leaking.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Line found leaking due to deterioration & rust. Same renewed with onboard fabricated new section. Leak rectified.","2022-04-23T23:59:35","NA","Completed","2022-03-24T23:59:35","No","No","No","Internal"]
[null,null,null,25404,36021,"0_Tue May 24 2022 21:46:31 GMT+0800","2022-03-26T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Emcy Fire Pump Vacuum Unit Priming Chamber Cover found wasted.","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","Renewed with new fabricated chamber.","2022-06-25T23:59:35","NA","Completed","2022-03-26T23:59:35","No","No","No","Internal"]
[null,null,null,25405,76875,"0_Tue May 24 2022 21:49:04 GMT+0800","2022-03-26T23:59:35","Observation","Ship Staff","Ship Staff Insp.","VRCS Return Line pipe section leaking.","Deck - Pipe / Fittings,Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","Return pipe section removed & weld repaired in ER Workshop. Installed back & tried out.","2022-06-25T23:59:35","NA","Completed","2022-03-26T23:59:35","No","No","No","Internal"]
[null,null,null,25409,20997,"24_Tue May 24 2022 22:06:38 GMT+0800","2022-03-26T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Water Ballast Tank #3P Bottom Line GRE Pipe leaking.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","Found pipe cracked & previously cold repaired. Shore team repaired the pipe with GRE pipe repair kit. tried out & found in order.","2022-04-22T23:59:35","","Completed","2022-04-07T23:59:35","No","No","No","Internal","Repair carried out by Shore Service team. Tested. No leak observed."]
[null,null,null,25394,36084,"24_Tue May 24 2022 15:20:44 GMT+0800","2022-03-27T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Main SW Pumps Discharge Manifold Pressure Gauge union has broken resulting in water leaking from the line.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","The leak was temporarily plugged with a wooden plug & reinforced it with a blank flange.. The gauge union flange & cock has been renewed. system back in use.","2022-06-26T23:59:35","NA","Completed","2022-05-04T23:59:35","No","No","No","Internal"]
[null,null,null,25395,57323,"0_Tue May 24 2022 15:23:19 GMT+0800","2022-03-27T23:59:35","Observation","Ship Staff","Ship Staff Insp.","HFO Purifier #1 Bowl Bowl Leakage.","E/R - Purifier","Eng. / Strg. Comp.","Equipment Related","","","","","Bowl opened up for inspection. Found the light liquid chamber o-ring damaged. Same renewed with new spare. Purifier tried out & in order.","2022-03-27T23:59:35","NA","Completed","2022-03-27T23:59:35","No","No","No","Internal"]
[null,null,null,25411,69897,"24_Tue May 24 2022 21:08:48 GMT+0800","2022-03-27T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Accommodation Gas Detection System is not showing any values.","Accommodation","Safety / LSA / FFA","Equipment Related","","","","","Complete Unit renewed with new received spare on 27-Apr-2022. A frame has been fabricated by shipstaff for installation. tried out & found working. Calibration gas required for making final calibrations to the system.","2022-07-15T23:59:35","RO DBAU220100","Completed","2022-04-17T23:59:35","No","No","No","Internal"]
[null,null,null,25414,63309,"24_Tue May 24 2022 21:54:39 GMT+0800","2022-03-27T23:59:35","Observation","Ship Staff","Ship Staff Insp.","AE #1 Crankcase Relief Valves Leaking","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Gaskets renewed. Leaks Rectified. RO raised for consumed spares.","2022-06-26T23:59:35","RO DBAU220068","Completed","2022-03-27T23:59:35","No","No","No","Internal"]
[null,null,null,25406,69564,"0_Tue May 24 2022 21:57:23 GMT+0800","2022-03-28T23:59:35","Observation","Ship Staff","Ship Staff Insp.","AE #2 Unit #2 Cylinder Head Water Leak","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Found Scavenge Inlet o-ring damaged. Cylinder Head replaced with overhauled spare. All o-rings/gaskets renewed. Rectified.","2022-06-27T23:59:35","NA","Completed","2022-03-28T23:59:35","No","No","No","Internal"]
[null,null,null,25407,46720,"0_Tue May 24 2022 21:59:36 GMT+0800","2022-03-29T23:59:35","Observation","Ship Staff","Ship Staff Insp.","AE #2 & #3 Crankcase Relief Door Gaskets leaking.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Gaskets renewed with new spares. Leaks rectified. RO raised for consumed spares.","2022-06-28T23:59:35","RO DBAU220068","Completed","2022-03-29T23:59:35","No","No","No","Internal"]
[null,null,null,25408,68341,"0_Tue May 24 2022 22:01:57 GMT+0800","2022-03-31T23:59:35","Observation","Ship Staff","Ship Staff Insp.","AE #2 Oil Max Pump Seal leaking.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Mechanical seal replaced with new spares. Leak rectified. RO raised for consumed spares.","2022-06-30T23:59:35","RO DBAU220055","Completed","2022-03-31T23:59:35","No","No","No","Internal"]
[null,null,null,25410,48941,"0_Tue May 24 2022 22:08:31 GMT+0800","2022-04-04T23:59:35","Observation","Ship Staff","Ship Staff Insp.","AHU #2 Drain Line found choked.","Accommodation,E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Same cleared.","2022-07-04T23:59:35","NA","Completed","2022-04-04T23:59:35","No","No","No","Internal"]
[null,null,null,25399,63418,"0_Tue May 24 2022 21:20:05 GMT+0800","2022-04-05T23:59:35","Observation","Ship Staff","Ship Staff Insp.","HFO Purifier #1 Leakage alarm.","E/R - Purifier","Eng. / Strg. Comp.","Equipment Related","","","","","Light liquid chamber o-ring supplied of incorrect size. Renewed with correct size o-ring available onboard. Purifier tried out & in order.","2022-07-05T23:59:35","NA","Completed","2022-04-05T23:59:35","No","No","No","Internal"]
[null,null,null,25412,12499,"24_Thu May 26 2022 21:12:03 GMT+0800","2022-04-09T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Cascade Tank Steam Heating Inlet Line leaking","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Flange gasket renewed. Leak Rectified.","2022-07-10T23:59:35","NA","Completed","2022-04-10T23:59:35","No","No","No","Internal"]
[null,null,null,25422,11760,"0_Sat May 28 2022 12:29:28 GMT+0800","2022-04-09T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Soot Collecting Tank found with water/soot collected.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Found the Outlet gate valve stuck in the closed position. This valve was heavily rusted/wasted. Renewed with onboard new spare. Rectified.","2022-07-20T23:59:35","NA","Completed","2022-04-20T23:59:35","No","No","No","Internal"]
[null,null,null,25396,77924,"0_Tue May 24 2022 15:36:51 GMT+0800","2022-04-10T23:59:35","Observation","Ship Staff","Ship Staff Insp.","FW & drinking found discoloured.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","FW Hydrophore Tank drained & manually cleaned. Water sterilizer filer also renewed. Accommodation FW now colourless. Sterilizer Filter ROB Nil. RO raised for the same.","2022-05-22T23:59:35","RO DBAU220113","Completed","2022-04-16T23:59:35","No","No","No","Internal"]
[null,null,null,25413,74034,"0_Thu May 26 2022 21:13:44 GMT+0800","2022-04-10T23:59:35","Observation","Ship Staff","Ship Staff Insp.","LT Cooler #2 SW Inlet Line Drain plug found wasted & leaking.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","LT Cooler drained. Plug renewed with new spare. Leak Rectified.","2022-04-10T23:59:35","NA","Completed","2022-04-10T23:59:35","No","No","No","Internal"]
[null,null,null,25366,14751,"24_Sat May 07 2022 14:04:54 GMT+0800","2022-04-12T23:59:35","Observation","Ship Staff","Ship Staff Insp.","HFO Purifier #2 found vibrating during operation.","E/R - Purifier","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Vertical shaft bearings found damaged. Same renewed. horizontal shaft also overhauled & bearings renewed. On opening the bowl, found the Bowl body & Distributor Locating pin housing damaged. Reconditioned bowl body & new fabricated distributor supplied. Distributor has slight grinding marks on the inner surface. Purifier boxed up & tried out. Currently in operation & confirmed in order after observing for 2 weeks.","2022-07-12T23:59:35","RO DBAU220095","Completed","2022-06-06T23:59:35","No","No","No","Internal","Please update on the status"]
[null,null,null,25371,81443,"24_Tue May 24 2022 17:16:16 GMT+0800","2022-04-13T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Main Cooling SW Pump #1 Vacuum Unit leaking","E/R - Pumps,LSA / FFA","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Overhauled and presently no leaks","2022-07-15T23:59:35","RO DBAU220069","Completed","2022-08-01T23:59:35","No","No","No","Internal","Spare parts have been supplied. Carry out the repair and revert."]
[null,null,null,25370,70326,"24_Tue May 24 2022 15:28:47 GMT+0800","2022-04-14T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Emcy Generator LO Analysis indicates \"Caution\".","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","LO Sump drained & manually cleaned. Flushed & refilled with fresh oil on 25-Apr-2022. Samples landed for shore analysis at Singapore for closure. Received analysis report & sample condition is satisfactory.","2022-06-21T23:59:35","NA","Completed","2022-06-11T23:59:35","No","No","No","Internal","Sump oil has been renewed and oil is new. As a precautionary measure vessel has been advised to land oil sample at Singapore for shore analysis."]
[null,null,null,25381,74767,"0_Tue May 24 2022 21:13:55 GMT+0800","2022-04-14T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Port side Lifeboat Battery Charging socket very tight.","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.28","Very High","","","eased up and made it free","2022-07-14T23:59:35","RO DBAU220101","Completed","2022-08-26T23:59:35","No","No","No","Internal"]
[null,null,null,25386,77629,"24_Sat May 28 2022 19:32:40 GMT+0800","2022-04-14T23:59:35","Observation","Ship Staff","Ship Staff Insp.","ME Unit #2 Shore CCM Test for Iron Content shows high","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","CCM test carried out onboard found to be less, hence reduced the feed from 1.25 to 1.2","2022-07-14T23:59:35","NA","Completed","2022-08-17T23:59:35","No","No","No","Internal","Last CCM test showed good improvement in Fe values. \nVessel has been asked to reduce CLO feed rate to 1.25 and observe."]
[null,null,null,25392,71684,"24_Sat May 07 2022 14:07:19 GMT+0800","2022-04-14T23:59:35","Observation","Ship Staff","Ship Staff Insp.","AE #3 Unit #5 Fuel Pump plunger-Barrel seized during operation.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Fuel pump replaced with overhauled spare. AE tried out & in order.","2022-07-14T23:59:35","NA","Completed","2022-04-14T23:59:35","No","No","No","Internal"]
[null,null,null,25393,93963,"24_Sat May 07 2022 14:10:58 GMT+0800","2022-04-14T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Emcy Generator Starting batteries casing cracked during routine starting.","Critical Equip.","Safety / LSA / FFA","Equipment Related","","","","","Batteries replaced with new received spares.","2022-07-14T23:59:35","RO DBAU220094","Completed","2022-04-15T23:59:35","No","No","No","Internal"]
[null,null,null,25415,64613,"0_Thu May 26 2022 21:15:44 GMT+0800","2022-04-14T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Purifier Room Aft Door found jammed in the closed position.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","Door lock removed & found spring latch had broken. Door handle mechanism  renewed with onboard spare. Rectified.","2022-07-10T23:59:35","NA","Completed","2022-04-14T23:59:35","No","No","No","Internal"]
[null,null,null,25416,25416,"0_Thu May 26 2022 21:17:27 GMT+0800","2022-04-15T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Emcy Fire Pump Discharge Line Drain Valve leaking.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Drain valve renewed with new spare. In order.","2022-07-16T23:59:35","NA","Completed","2022-04-16T23:59:35","No","No","No","Internal"]
[null,null,null,25374,39428,"0_Thu May 26 2022 21:24:04 GMT+0800","2022-04-16T23:59:35","Observation","Ship Staff","Ship Staff Insp.","AE #1 Unit #1,#3, #4 & #6 Fuel Pump HP Pipes Leaking.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Sealing face lapped but the leak still persists. Spare HP pipes received. Renewed the same. Tried out & No leaks observed.","2022-07-16T23:59:35","RO DBAU220092","Completed","2022-05-26T23:59:35","No","No","No","Internal"]
[null,null,null,25375,87425,"0_Thu May 26 2022 21:26:03 GMT+0800","2022-04-16T23:59:35","Observation","Ship Staff","Ship Staff Insp.","AE #3 Unit #3 & #6 Fuel Pump HP Pipes leaking from Face seating","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Pipe seating face lapped but leak still persists. Received HP pipes. Renewed for the leaking units. Fuel valves also renewed as the seating face for the HP pipes also found damaged. All Pipe leaks rectified.","2022-07-16T23:59:35","RO DBAU220092","Completed","2022-06-23T23:59:35","No","No","No","Internal"]
[null,null,null,25419,22542,"0_Thu May 26 2022 21:34:07 GMT+0800","2022-04-17T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Accommodation AC Compressor #2 Starter Switch not working.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Starter switch renewed with new spare. Rectified.","2022-07-17T23:59:35","NA","Completed","2022-04-17T23:59:35","No","No","No","Internal"]
[null,null,null,25420,30965,"0_Thu May 26 2022 21:36:02 GMT+0800","2022-04-17T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Pump room lighting found fused in 3 locations.","Elect. Mach. & Equip.","Cargo / Ballast Systems","Equipment Related","","","","","Light holders found deteriorated. Holders renewed with new spares. Rectified.","2022-08-18T23:59:35","NA","Completed","2022-04-18T23:59:35","No","No","No","Internal"]
[null,null,null,27481,63830,"24_Mon Oct 03 2022 15:23:32 GMT+0800","2022-04-17T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Few standby pumps in ECR panel found to be operating in MANUAL mode. All pumps should be in Auto mode and second pump in Standby","E/R - Pumps","Eng. / Strg. Comp.","Human Error","10.32","Very High","","","All pumps changed over to Auto and Second pumps put in Auto. All Engine staff made aware to follow the same.","2022-04-23T23:59:35","","Completed","2022-04-19T23:59:35","No","No","No","Internal"]
[null,null,null,27482,58815,"24_Mon Oct 03 2022 15:26:30 GMT+0800","2022-04-17T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Old MSDS Sheets are still in use for chemicals in the chemical locker. The latest version of MSDS to be used for all gases and chemicals.","Miscellaneous","ISM Related","Human Error","5.46","Medium","","","Renewed all chemical and gases MSDS which are more than 5years old.","2022-05-17T23:59:35","","Completed","2022-05-10T23:59:35","No","No","No","Internal"]
[null,null,null,27483,38151,"24_Mon Oct 03 2022 16:19:05 GMT+0800","2022-04-17T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Light casing on poopdeck was found to be damaged and is to be renewed.","Elect. Mach. & Equip.","General Appearance","Equipment Related","11.10","Medium","","","Renewed the damaged light casing.","2022-05-16T23:59:35","","Completed","2022-04-23T23:59:35","No","No","No","Internal"]
[null,null,null,27484,13726,"24_Mon Oct 03 2022 16:01:04 GMT+0800","2022-04-17T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ER Toolbox meeting form not being filled up on daily basis","Documentation","ISM Related","Behaviour Based","10.32","Very High","","","Filled on daily basis and filed.","2022-04-23T23:59:35","","Completed","2022-04-19T23:59:35","No","No","No","Internal"]
[null,null,null,27485,87508,"24_Mon Oct 03 2022 15:52:21 GMT+0800","2022-04-17T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Insulation missing on both M/E turbocharger exhaust pipelines.","E/R - Main Engine","ISM Related","Human Error","10.32","Very High","","","Fitted new insulation on the exhaust pipes and flanges.","2022-07-16T23:59:35","","Completed","2022-08-30T23:59:35","No","No","No","Internal"]
[null,null,null,27486,75807,"24_Mon Oct 03 2022 15:32:54 GMT+0800","2022-04-17T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","M/E unit no.7 fuel pump drain valve found leaking. Vessel to raise RO for new valve and renew the same.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Renewed the valve and found no leaks.","2022-07-16T23:59:35","DBAU220122","Completed","2022-09-16T23:59:35","No","No","No","Internal"]
[null,null,null,27487,43565,"24_Mon Oct 03 2022 15:58:02 GMT+0800","2022-04-17T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","EGCS Data not being entered in Engine logbook. Stamp found missing onboard. The vessel to order a stamp from the office.","E/R - Aux. Mach.","ISM Related","Human Error","10.5","Low","","","Stamp found onboard and started entering the data in Engine Log book.","2022-05-08T23:59:35","","Completed","2022-04-29T23:59:35","No","No","No","Internal"]
[null,null,null,27488,44222,"24_Mon Oct 03 2022 15:38:30 GMT+0800","2022-04-17T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Insulation mats missing at several places infront of electrical panels.","Elect. Mach. & Equip.","ISM Related","Human Error","10.24","Low","","","New mats fitted at places where the mats are missing.","2022-05-16T23:59:35","","Completed","2022-04-24T23:59:35","No","No","No","Internal"]
[null,null,null,27489,18710,"24_Mon Oct 03 2022 16:15:18 GMT+0800","2022-04-17T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","EGCS MGPS control panel found not operational.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Raised RO for new control panel and renewed the same, working satisfactorily.","2022-07-16T23:59:35","","Completed","2022-08-10T23:59:35","No","No","No","Internal"]
[null,null,null,27490,85188,"24_Mon Oct 03 2022 16:12:34 GMT+0800","2022-04-17T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Pressure release valves for the sounding pipes in the engine room need maintenance as several of them found in stuck condition.","E/R - Pipes/ valves & fittings","Structural Condn. / WT integrity ","Human Error","10.26","High","","","All the valves eased up for correct operation. found to be working in order.","2022-05-16T23:59:35","","Completed","2022-05-12T23:59:35","No","No","No","Internal"]
[null,null,null,27491,66691,"24_Mon Oct 03 2022 16:08:34 GMT+0800","2022-04-17T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Color coding of valves not in place in the engine room","E/R - Pipes/ valves & fittings","General Appearance","Knowledge Based","10.32","Very High","","","All valves in E/R colour coded as per the medium in use. ","2022-07-16T23:59:35","","Completed","2022-07-07T23:59:35","No","No","No","Internal"]
[null,null,null,27492,73277,"24_Mon Oct 03 2022 21:06:36 GMT+0800","2022-04-17T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Broom Locker on upper deck needs to be arranged and inventory to be taken.","Accommodation","General Appearance","Inappropriate Procedure","5.11","Low","","","Broom Locker cleaned and stores arranged inventory taken","2022-05-01T23:59:35","","Completed","2022-04-29T23:59:35","No","No","No","Internal"]
[null,null,null,25445,36352,"24_Tue May 10 2022 17:36:03 GMT+0800","2022-04-17T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","AE #1 All Fuel pumps Seized.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related,Industry Issue","","","","","All the Fuel pumps found seized. Renewed with onboard new spares. AE #2 changed over to HFO. In use.","2022-04-17T23:59:35","","Completed","2022-05-19T23:59:35","No","No","No","Internal"]
[null,null,null,27493,55739,"24_Mon Oct 03 2022 20:42:25 GMT+0800","2022-04-17T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Stay Wire for forward and midships mast in bad condition","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.5","Medium","","","Stay wire for forward and midship mast wire brushed, inspected found good condition.  Lubrication carried out.","2022-05-17T23:59:35","","Completed","2022-08-05T23:59:35","No","No","No","Internal"]
[null,null,null,25446,40092,"24_Sat May 28 2022 19:07:06 GMT+0800","2022-04-17T23:59:35","Observation","Ship Staff","Ship Staff Insp.","FW Tank (Port) found with salty taste & high chlorides.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Found the FWG Ejector pump line from Fire & GS Pump valve not holding. This resulted in SW going in the FW Tank when the FWG was stopped & fire pump was running. Line blanked. FW Tank Port drained completely & inspcted. Tank refilled with FW from FWG. Rectified.","2022-04-17T23:59:35","NA","Completed","2022-05-19T23:59:35","No","No","No","Internal"]
[null,null,null,27494,96074,"24_Mon Oct 03 2022 20:38:37 GMT+0800","2022-04-17T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Cover for SOPEP drums on midships locker found to be broken.  Requisition for spare drum to be raised and to be replaced.","Miscellaneous","MARPOL Related","Equipment Related","6.1","Medium","","","Stores received and replaced.","2022-06-17T23:59:35","DBAU 220107","Completed","2022-06-05T23:59:35","No","No","No","Internal"]
[null,null,null,27495,97572,"24_Mon Oct 03 2022 16:05:00 GMT+0800","2022-04-17T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","LO Drums in the steering gear room are not secured for heavy weather. Drums are placed directly on the floor.","Miscellaneous","Eng. / Strg. Comp.","Behaviour Based","10.29","Medium","","","Drums placed on top of the wooden pallet, secured properly with proper wire rope.","2022-05-16T23:59:35","","Completed","2022-05-05T23:59:35","No","No","No","Internal"]
[null,null,null,27496,44159,"24_Mon Oct 03 2022 20:24:58 GMT+0800","2022-04-17T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Food Menu could not be located for both Officers and Crew Mess Room.","Accommodation","MLC Related","Inappropriate Procedure","","","","","Food menu prepared and displayed on Officers and crew messroom.","2022-05-01T23:59:35","","Completed","2022-04-28T23:59:35","No","No","No","Internal"]
[null,null,null,27498,75167,"24_Mon Oct 03 2022 20:29:41 GMT+0800","2022-04-17T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Common Store on Poop deck not arranged properly and found all spares  mixed up.   Store to be arranged and inventory to be taken.","Accommodation","General Appearance","Behaviour Based,Inappropriate Procedure","5.11","Low","","","Common stores cleaned arranged and inventory taken","2022-05-17T23:59:35","","Completed","2022-07-04T23:59:35","No","No","No","Internal"]
[null,null,null,27499,92891,"24_Mon Oct 03 2022 15:55:51 GMT+0800","2022-04-17T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Root valve pipeline for AE EGCS Pressrue transmitter on ECR Platform near no.2 Aux. boiler found to be damaged.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Renewed the line from spare and checked for leaks found no leaks.","2022-05-03T23:59:35","","Completed","2022-04-23T23:59:35","No","No","No","Internal"]
[null,null,null,27500,84432,"24_Mon Oct 03 2022 20:59:12 GMT+0800","2022-04-17T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Few VRCS hydraulic lines and midship lines on deck need immediate attention and need to be renewed asap.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","11.4","Very High","","","Corroded VRCS line renewed with new pipe.  And Pipe tested found holding good.","2022-07-17T23:59:35","","Completed","2022-05-13T23:59:35","No","No","No","Internal"]
[null,null,null,27519,54431,"24_Mon Oct 03 2022 21:17:56 GMT+0800","2022-04-17T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Anchor wash branch pipes for both the Port and starboard side in the fore castle store damaged.  Temporary repairs have been carried out.  All damaged pipe sections need to be renewed.","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","Equipment Related","11.4","Very High","","","All damaged pipe section removed and repaired","2022-06-17T23:59:35","","Completed","2022-06-15T23:59:35","No","No","No","Internal"]
[null,null,null,25372,47628,"0_Tue May 24 2022 21:11:02 GMT+0800","2022-04-18T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Accommodation Gas Detection system Calibration Gas ROB Nil.","Accommodation","Safety / LSA / FFA","Equipment Related","5.21","Medium","","","Rec'd Calibration gas at Singapore. ","2022-07-18T23:59:35","RO DBAU220100","Completed","2023-01-13T23:59:35","No","No","No","Internal"]
[null,null,null,25444,85536,"24_Tue May 24 2022 15:41:30 GMT+0800","2022-04-18T23:59:35","Observation","Ship Staff","Ship Staff Insp.","AE #2 all fuel pumps Seized.","E/R - Aux. Engine","Eng. / Strg. Comp.","Industry Issue","","","","","All fuel pumps renewed with overhauled ones with new plunger barrels. This is due to Bad quality HFO supplied at Singapore on 06-Mar-2022. ","2022-04-19T23:59:35","NA","Completed","2022-04-19T23:59:35","No","No","No","Internal"]
[null,null,null,25368,49354,"24_Tue May 10 2022 17:41:14 GMT+0800","2022-04-19T23:59:35","Observation","Ship Staff","Ship Staff Insp.","AE #1 Unit #4 Fuel Pump outlet Flange leak.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Oil found leaking heavily from AE#1 Fuel pump inlet flange. Gasket renewed with onboard oil gasket. Reinforced high temp oil gaskets are required & have been ordered, Same received at Singapore. Gaskets renewed for leaking Flanges. AE Tried out & No leaks observed.","2022-07-19T23:59:35","RO DBAU220103","Completed","2022-05-26T23:59:35","No","No","No","Internal","Will be supplied at SIngapore"]
[null,null,null,25373,42921,"24_Tue May 24 2022 21:17:30 GMT+0800","2022-04-19T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Emcy Generator Starting Battery Isolator rated more than battery starting current.","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","Battery fit with 120Ah Isolator. Batteries rated at 100Ah. RO raised for correct rating of battery isolator & received the same at Singapore. Installed & tried out. Found in order.","2022-07-19T23:59:35","RO DBAU220116","Completed","2022-06-08T23:59:35","No","No","No","Internal","RO approved and will be supplied in Singapore."]
[null,null,null,25377,51415,"0_Sat May 28 2022 12:26:30 GMT+0800","2022-04-19T23:59:35","Observation","Ship Staff","Ship Staff Insp.","04 Nos. Floodlights of Sodium Vapour Lamps found with decayed bodies.","Elect. Mach. & Equip.","Navigation","Equipment Related","11.11","Very High","","","Renewed the light with base.","2022-07-19T23:59:35","RO DBAU220101","Completed","2022-09-04T23:59:35","No","No","No","Internal"]
[null,null,null,25397,63898,"0_Tue May 24 2022 16:03:56 GMT+0800","2022-04-19T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Fire Line Fwd of Accommodation  found with pin hole leak.","LSA / FFA,Deck - Pipe / Fittings","Safety / LSA / FFA","Equipment Related","","","","","Fire Line section removed & shifted to ER Workshop for repair. Pipe repaired bywelding & re-installed back. Tried out & in use.","2022-04-21T23:59:35","NA","Completed","2022-04-19T23:59:35","No","No","No","Internal"]
[null,null,null,25398,47422,"0_Tue May 24 2022 17:10:36 GMT+0800","2022-04-19T23:59:35","Observation","Ship Staff","Ship Staff Insp.","ME FO Auto Backwash filter found with sludge/particle deposits.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Industry Issue","","","","","Filter elements cleaned & boxed up. Filter sludge due to the bad quality fuel supplied at Singapore on 06-Mar-2022.","2022-07-22T23:59:35","NA","Completed","2022-04-19T23:59:35","No","No","No","Internal"]
[null,null,null,25421,77520,"24_Sat May 28 2022 12:20:50 GMT+0800","2022-04-19T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Anchor Light not operational & showing low insulation alarm.","Navigation - Others,Elect. Mach. & Equip.","Navigation","Equipment Related","","","","","Anchor Light to Junction Box cable found broken due to deterioration. Enitre length of cable replaced with new spare.  Rectified.","2022-07-19T23:59:35","NA","Completed","2022-04-19T23:59:35","No","No","No","Internal"]
[null,null,null,25369,72878,"24_Tue May 10 2022 17:45:47 GMT+0800","2022-04-20T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Accommodation AC Compressor #2 Motor found with increased vibrations.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Received motor on 23/08/2022 to be renewed at convenient opportunity. Presently working satisfactorily.","2022-07-20T23:59:35","RO DBAU220149","Completed",null,"No","No","No","Internal","Send a descriptive report to office on the motor condition with attached photographs."]
[null,null,null,25417,67889,"0_Thu May 26 2022 21:19:25 GMT+0800","2022-04-20T23:59:35","Observation","Ship Staff","Ship Staff Insp.","FW Hydrophore Tank Gauge Glass found leaking.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Gauge Glass renewed with new spare. Rectified.","2022-07-20T23:59:35","NA","Completed","2022-04-20T23:59:35","No","No","No","Internal"]
[null,null,null,25418,52677,"0_Thu May 26 2022 21:28:50 GMT+0800","2022-04-22T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Fish Room temperature not maintained.","Accommodation,Elect. Mach. & Equip.","MLC Related","Equipment Related","","","","","Found Fish room thermostat malfunctioning. Same renewed with new spare. Rectified.","2022-07-24T23:59:35","NA","Completed","2022-04-23T23:59:35","No","No","No","Internal"]
[null,null,null,25423,54027,"0_Sat May 28 2022 12:36:15 GMT+0800","2022-04-25T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Main Engine unable to operate at Dead slow Ahead after changeover to LSMGO.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","While vessel was approaching Jebel Dhana for Loading, Main engine shut down when at Dead Slow. Found the ME unable to fire on LSMGO in ahead & astern direction. Only firing in ahead direction with addtional fuel. ME operated on Local maneouvring & drifted to troubleshoot. Decided to anchor the vessel at Khorfakkan to rectify. MAN ES Service Team arranged For Fuel Pump Overhaul. Found all the Fuel Pumps plunger barrels worn out due to bad quality fuel. All fuel pump plunger barrels renewed with new spare. ME tried out in presence of MAN Technians & Class Surveyor. Found in order.","2022-05-02T23:59:35","","Completed","2022-05-01T23:59:35","No","No","No","Internal"]
[null,null,null,25367,43021,"24_Tue May 10 2022 17:32:48 GMT+0800","2022-04-30T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Port Windlass unable to heave up the anchor at 4 cables.","Deck - Mooring Machinery","Mooring","Equipment Related","9.20","Medium","","","Tried out at singapore found working satisfactorily.","2022-05-01T23:59:35","RO DBAU220112","Completed","2022-10-25T23:59:35","No","No","No","Internal","PO raised and will be supplied."]
[null,null,null,25378,96555,"0_Sat May 28 2022 12:40:20 GMT+0800","2022-04-30T23:59:35","Observation","Ship Staff","Ship Staff Insp.","HFO Settling & Service Tank Cleaning required due to Bad quality fuel.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","HFO Settling & Service Tank contents tranferred to HFO Bunker Tank #2 Stbd. HFO Settl & Serv Tanks manually cleaned & inspected on 13-May-2022. HFO Bunker Tank #2 stbd put in use as GCMS test came back satisfactory.","2022-07-31T23:59:35","NA","Completed","2022-06-02T23:59:35","No","No","No","Internal","GCMS test of HFO 2 Starboard was carried out and came out to be Satisfactory. Start consuming bunkers after discharge operations at Rayong"]
[null,null,null,25382,56470,"0_Sat May 28 2022 17:52:58 GMT+0800","2022-04-30T23:59:35","Observation","Ship Staff","Ship Staff Insp.","ME All units Fuel Pumps Erosion plugs found with pitting.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Renewed all erosion plugs from spare. ","2022-07-31T23:59:35","RO DBAU220104","Completed","2022-09-28T23:59:35","No","No","No","Internal","PO raised and will be supplied to the vessel at next convenient port."]
[null,null,null,25433,74392,"0_Sat May 28 2022 12:42:30 GMT+0800","2022-05-01T23:59:35","Observation","Ship Staff","Ship Staff Insp.","ECR AC Found with icing on the Evaporator.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","Both AC belts renewed as they were found worn out. Gas charged. System leak tested & tried out. operating satisfactorily.","2022-08-01T23:59:35","NA","Completed","2022-05-01T23:59:35","No","No","No","Internal"]
[null,null,null,25427,29918,"0_Sat May 28 2022 12:58:30 GMT+0800","2022-05-02T23:59:35","Observation","Ship Staff","Ship Staff Insp.","COT #1 Stbd Temperature showing fault/erratic.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","Opened Transmitter Unit & found with water ingress. Replaced cover gasket. tried out & found in order.","2022-08-02T23:59:35","NA","Completed","2022-05-02T23:59:35","No","No","No","Internal"]
[null,null,null,25432,98437,"24_Sat May 28 2022 12:48:53 GMT+0800","2022-05-02T23:59:35","Observation","Ship Staff","Ship Staff Insp.","HFO Settl & Serv Tank Vent Line found choked.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Pipe Line manually cleared. Rectfied.","2022-08-02T23:59:35","NA","Completed","2022-05-04T23:59:35","No","No","No","Internal"]
[null,null,null,25426,20854,"0_Sat May 28 2022 12:56:15 GMT+0800","2022-05-03T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Ballast Tank Ullage System showing erratic readings.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","Found air leak in the transmitter conrtrol panel. leak rectified. All Tank Level gauges calibrated. System in order & in use.","2022-08-03T23:59:35","NA","Completed","2022-05-03T23:59:35","No","No","No","Internal"]
[null,null,null,25424,58295,"0_Sat May 28 2022 12:50:42 GMT+0800","2022-05-04T23:59:35","Observation","Ship Staff","Ship Staff Insp.","VRCS return line leaking.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","","","","","Pipeline Found with pin hole leak. Rectified by welding in ER Workshop.","2022-08-04T23:59:35","NA","Completed","2022-05-05T23:59:35","No","No","No","Internal"]
[null,null,null,25425,40316,"0_Sat May 28 2022 12:53:37 GMT+0800","2022-05-04T23:59:35","Observation","Ship Staff","Ship Staff Insp.","3rd Officer Cabin Vacuum Toilet not working.","Accommodation","MLC Related","Equipment Related","","","","","Found the flush valve & control mechanism defective. Same renewed with new spare. Rectified.","2022-08-04T23:59:35","NA","Completed","2022-05-05T23:59:35","No","No","No","Internal"]
[null,null,null,25379,42194,"0_Sat May 28 2022 13:01:11 GMT+0800","2022-05-07T23:59:35","Observation","Ship Staff","Ship Staff Insp.","VRCS Unit LO Tank level found dropping. About 500ltrs of oil topped up.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.21","High","","","Leak found in the Solenoid block of CL230. Same rectified by o-ring renewal. Suspect leak in Drop Valves CL250 & CL252. Under observation.\nCL250 and CL 252 kept pressurized open during last loading operation at Rastanurah.  No leaks observed. ","2022-08-07T23:59:35","","Completed","2022-08-22T23:59:35","No","No","No","Internal","Status to be advised."]
[null,null,null,25383,19630,"0_Sat May 28 2022 18:10:18 GMT+0800","2022-05-07T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Bosun Store Supply Fan found operating with noise.","Deck - Machinery","General Appearance","Equipment Related","","","","","Supply fan removed & brought to Workshop. Fan Impeller is stuck on the shaft.  Extractor fabricated for removal. Bearings renewed & motor installed back. Tried out & in order.","2022-08-07T23:59:35","NA","Completed","2022-06-01T23:59:35","No","No","No","Internal","Complete this on priority and advise the status."]
[null,null,null,25429,43744,"24_Sat May 28 2022 17:39:10 GMT+0800","2022-05-07T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Feed Pipe from WO Sludge Pump to Incinerator Waste Oil Tank choked.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Pipe removed & cleared manually. Installed back & tried out. Line cleared.","2022-08-09T23:59:35","NA","Completed","2022-05-09T23:59:35","No","No","No","Internal"]
[null,null,null,25380,92570,"0_Sat May 28 2022 13:03:55 GMT+0800","2022-05-08T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Stbd Bilge Well found with oil.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Found the Main Air Compressor & Bottles drain directly into the Bilge well. Cascade chamber fabricated & installed on the tank top to resolve this issue. the cascade tank fabricated is too small to accommodate the high line pressure. The bilge well has been cleaned & oil free. It is now being regularly skimmed & oil cleared.","2022-08-08T23:59:35","NA","Completed","2022-07-03T23:59:35","No","No","No","Internal","Please send photos to office for review. Send us the current status now."]
[null,null,null,25428,98108,"0_Sat May 28 2022 13:06:19 GMT+0800","2022-05-09T23:59:35","Observation","Ship Staff","Ship Staff Insp.","ME FO Supply Pump #1 Leak from mechanical seal.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","","","","","Seal renewed with new spare. RO raised for consumed spares.","2022-08-09T23:59:35","RO DBAU220058","Completed",null,"No","No","No","Internal"]
[null,null,null,25384,59695,"24_Sat May 28 2022 19:16:52 GMT+0800","2022-05-10T23:59:35","Observation","Ship Staff","Ship Staff Insp.","BWTS Filter #2 Outlet valve PT-2212 not showing fully shut on the MIMC panel.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.80","Medium","","","Valve showing fully shut locally & operating as per command given. MIMIC panel not displaying valve full shut & showing \"F/U Valves Time Out\" Alarm.\nService engineer attended the vessel.  Tested the equipmnet, even though the valve is actually closing and opening correctly, the mmic indication is not showing in fully close position.  And BWTS  functions is working correctly.","2022-08-10T23:59:35","NA","Completed","2022-09-16T23:59:35","No","No","No","Internal","Query sent to makers for advise. Have arranged for SE attendance in Singapore."]
[null,null,null,25385,91967,"0_Sat May 28 2022 19:22:40 GMT+0800","2022-05-10T23:59:35","Observation","Ship Staff","Ship Staff Insp.","BWTS mimic panel found not giving audible alarm.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","The Mimic panel Computer restarted. The BWTS Unit Restarted. Issue not resolved. Maker advised to restart the system & increase the volume via windows. same carried out & now system audio alarm is working.","2022-08-10T23:59:35","NA","Completed","2022-06-03T23:59:35","No","No","No","Internal"]
[null,null,null,25430,50800,"0_Sat May 28 2022 17:41:53 GMT+0800","2022-05-10T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Mooring Winch M7 Hydraulic Oil Outlet line found leaking.","Deck - Mooring Machinery","Mooring","Equipment Related","","","","","Pipe section removed & repaired in ER Workshop by welding. Installed back & tried out. Rectified.","2022-08-10T23:59:35","NA","Completed","2022-05-10T23:59:35","No","No","No","Internal"]
[null,null,null,25439,20614,"24_Sat May 28 2022 18:14:18 GMT+0800","2022-05-10T23:59:35","Observation","Ship Staff","Ship Staff Insp.","FWD Whistle found not operational.","Navigation - Others","Navigation","Equipment Related","","","","","Whistle found tripped on overload. On investigation, found the End Cover bolts had come loose & resulted in overload trip. Same re-tightened with spring washers. tried out & found in order.","2022-08-10T23:59:35","NA","Completed","2022-05-11T23:59:35","No","No","No","Internal"]
[null,null,null,25443,78092,"0_Sat May 28 2022 19:20:33 GMT+0800","2022-05-10T23:59:35","Observation","Ship Staff","Ship Staff Insp.","BWTS Loop #1 Recirc Valve BA-511 not operating as per command.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","Valve found operating in reverse to the command given. This was happening in BWTS & VRCS mode. Valve Indicator hydraulic block found installed incorrectly. installed correctly. Valve operating as per command.","2022-08-10T23:59:35","NA","Completed","2022-05-14T23:59:35","No","No","No","Internal"]
[null,null,null,25376,82039,"0_Thu May 26 2022 21:32:12 GMT+0800","2022-05-11T23:59:35","Observation","Ship Staff","Ship Staff Insp.","All Mooring Winch hydraulic brake systems not working smoothly.","Deck - Mooring Machinery","Mooring","Equipment Related","9.14","Medium","","","Vessel has overhauled all mooring winch brake arrangement blocks.","2022-08-11T23:59:35","RO DBAU220132","Completed","2022-11-24T23:59:35","No","No","No","Internal","How many have been overhauled? Please specify as per Winch number and revert with results for individual winch braking system."]
[null,null,null,25431,47676,"0_Sat May 28 2022 17:45:22 GMT+0800","2022-05-11T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Stbd Windlass Drum Wire Entangled.","Deck - Mooring Machinery","Mooring","Human Error","","","","","Wire severely entangled. Cut using Gas torch. Renewed with onboard new spare. RO raised for consumed wire rope.","2022-08-11T23:59:35","RO DBAU220114","Completed","2022-05-11T23:59:35","No","No","No","Internal"]
[null,null,null,25434,70959,"0_Sat May 28 2022 17:49:28 GMT+0800","2022-05-11T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Control & Service Air Compressors tripped due to high temperature.","E/R - Aux. Mach.","Eng. / Strg. Comp.","External Factors","","","","","High Temp. alarm received because of clogging of suction filters due to a Dust storm. Entire engine room also covered with dust. All suction filters cleaned & compressors put back in service. engine room cleaned & all dust removed.","2022-08-11T23:59:35","NA","Completed","2022-05-12T23:59:35","No","No","No","Internal"]
[null,null,null,25435,47402,"0_Sat May 28 2022 17:54:27 GMT+0800","2022-05-11T23:59:35","Observation","Ship Staff","Ship Staff Insp.","ME Unit #1 & #4 Erosion Plug leaking.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Plug gaskets renewed with new spare. Rectified.","2022-08-12T23:59:35","NA","Completed","2022-05-12T23:59:35","No","No","No","Internal"]
[null,null,null,25437,38834,"0_Sat May 28 2022 18:03:15 GMT+0800","2022-05-11T23:59:35","Observation","Ship Staff","Ship Staff Insp.","ME Unit #3 & #5 Fuel Pump Inlet Flange leaking.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Flange gasket renewed. Rectified.","2022-08-12T23:59:35","NA","Completed","2022-05-12T23:59:35","No","No","No","Internal"]
[null,null,null,25388,58436,"24_Sun May 29 2022 17:56:04 GMT+0800","2022-05-12T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Both Ballast eductors not working","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.80","Medium","","","Both Eductor unit opened for inspection, condition checked and inspected, no foreign material found, nozzle and pipe line found clear. After boxing back both eductors were tried out, even though negative suction -50 and discharge pressure of 5.8 bars was there but sounding of the tanks remain unchanged.\nSuspect Ballast discharge NRV BA BA 521 and No2 Ballast Drive 519, Or No2 Eductor Suction Valve BA 518 and No2 Ballast discharge side for filling tanks BA 515 leaking and Eductor suction not creating enough vaccum. ","2022-08-11T23:59:35","","Completed","2022-09-23T23:59:35","No","No","No","Internal","What is the status and progress of the investigation ? What are the findings? \nHas inspection been carried out?"]
[null,null,null,25436,24255,"0_Sat May 28 2022 18:01:30 GMT+0800","2022-05-12T23:59:35","Observation","Ship Staff","Ship Staff Insp.","ME Unit #2 Fuel Pump Aft HP Pipe leaking.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Aft HP Pipe sealing face cleaned. O-ring renewed with new spare.  Rectified.","2022-08-12T23:59:35","NA","Completed","2022-05-12T23:59:35","No","No","No","Internal"]
[null,null,null,25438,35406,"0_Sat May 28 2022 18:06:08 GMT+0800","2022-05-12T23:59:35","Observation","Ship Staff","Ship Staff Insp.","ME Unit #6 Fuel Pump HP Pipe leak off Line Pipe found cracked.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Same renewed with new fabricated line. Rectified.","2022-08-12T23:59:35","NA","Completed","2022-05-12T23:59:35","No","No","No","Internal"]
[null,null,null,25441,57735,"0_Sat May 28 2022 18:50:12 GMT+0800","2022-05-12T23:59:35","Observation","Ship Staff","Ship Staff Insp.","ME Turbocharger #1 Grit Wash line found choked.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Line & unit removed & manually cleared. Boxed-up, tried out & found in order.","2022-08-13T23:59:35","NA","Completed","2022-05-13T23:59:35","No","No","No","Internal"]
[null,null,null,25442,72860,"0_Sat May 28 2022 18:53:28 GMT+0800","2022-05-14T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Boiler Feed Water Pump #2 found with vibration during operation.","E/R - Aux. Mach.,E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","Pump overhauled. Found Bearing damaged & shaft sleeve worn with grooving. Bearings, Mech Seal & Shaft Sleeve renewed with new spare. RO to be raised for consumed spares.","2022-08-14T23:59:35","","Completed","2022-05-16T23:59:35","No","No","No","Internal"]
[null,null,null,25447,34780,"0_Sat May 28 2022 19:09:42 GMT+0800","2022-05-15T23:59:35","Observation","Ship Staff","Ship Staff Insp.","IG Scrubber Tower Flue Gas Nozzles flange found leaking.","Inert Gas","Cargo / Ballast Systems","Equipment Related","","","","","Observed the flange gasket wasted. Same renewed with new fabricated spare. Rectified.","2022-08-15T23:59:35","NA","Completed","2022-05-19T23:59:35","No","No","No","Internal"]
[null,null,null,25440,84701,"24_Sat May 28 2022 18:48:11 GMT+0800","2022-05-16T23:59:35","Observation","Ship Staff","Ship Staff Insp.","EGCS Room Lights found fused in multiple locations.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Light holders found defective. Same renewed with new spares. Rectified.","2022-08-16T23:59:35","NA","Completed","2022-05-17T23:59:35","No","No","No","Internal"]
[null,null,null,25448,12328,"24_Sun May 29 2022 19:44:11 GMT+0800","2022-05-18T23:59:35","Observation","Ship Staff","Ship Staff Insp.","IG Scrubber Inlet Ventury Unit SW Leak.","Inert Gas","Cargo / Ballast Systems","Equipment Related","","","","","Flange Gasket found deteriorated. Same renewed with new fabricated spare.","2022-08-18T23:59:35","NA","Completed","2022-05-19T23:59:35","No","No","No","Internal"]
[null,null,null,26038,69981,"24_Sat Jun 25 2022 13:29:41 GMT+0800","2022-05-19T23:59:35","Observation","Ship Staff","Ship Staff Insp.","ME Unit #2 & #7 Fuel Pump Inlet Valves not holding.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Renewed all the valves.","2022-09-19T23:59:35","RO DBAU220122","Completed","2022-09-28T23:59:35","No","No","No","Internal"]
[null,null,null,26039,55335,"24_Sat Jun 25 2022 13:33:06 GMT+0800","2022-05-19T23:59:35","Observation","Ship Staff","Ship Staff Insp.","ME Unit #7 Fuel Pump Drain Valve not holding.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Renewed the valve","2022-08-19T23:59:35","RO DBAU220122","Completed","2022-09-16T23:59:35","No","No","No","Internal"]
[null,null,null,25390,37159,"24_Sun May 29 2022 19:47:28 GMT+0800","2022-05-20T23:59:35","Observation","Ship Staff","Ship Staff Insp.","S-band Radar found not transmitting.","Navigation - RADAR","Navigation","Equipment Related","","","","","Radar Scanner unit not rotating as no 12V supply to the contactor.  Following parts renewed with new spares. Bearing PCB, Trigger PCB, Input PCB & P M Cable S. Radar issue resolved after Shore Service attendance at Singapore on 13-Jun-2022.","2022-08-16T23:59:35","","Completed","2022-06-04T23:59:35","No","No","No","Internal","Trouble shooting in progress with Makers consultation.\nService attendance has been arranged at Singapore. Flag dispensation taken and same has been approved."]
[null,null,null,26067,75076,"24_Sat Jun 25 2022 13:37:23 GMT+0800","2022-05-20T23:59:35","Observation","Ship Staff","Ship Staff Insp.","HFO Service Tank Steam Heating Inlet & Bypass valve not holding.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Ro raised for spares. Received the same & installed. Tried out & no leaks observed. In use.","2022-08-20T23:59:35","RO DBAU220120","Completed","2022-06-03T23:59:35","No","No","No","Internal"]
[null,null,null,26051,19688,"0_Thu Jun 23 2022 17:19:29 GMT+0800","2022-05-21T23:59:35","Observation","Ship Staff","Ship Staff Insp.","HFO Settling Tank High Level Float not functioning.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Float switch found defective. Same renewed with onboard spare. Tried out & found in order.","2022-08-21T23:59:35","NA","Completed","2022-05-21T23:59:35","No","No","No","Internal"]
[null,null,null,26047,44501,"24_Thu Jun 23 2022 17:07:25 GMT+0800","2022-05-22T23:59:35","Observation","Ship Staff","Ship Staff Insp.","AE #3 Unit #3 Fuel Pump Outlet Flange gasket found damaged.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Same replaced with new gasket. In order.","2022-08-22T23:59:35","NA","Completed","2022-05-22T23:59:35","No","No","No","Internal"]
[null,null,null,26048,36403,"0_Thu Jun 23 2022 17:10:10 GMT+0800","2022-05-22T23:59:35","Observation","Ship Staff","Ship Staff Insp.","AE #3 EGCS Pressure Transmitter pipe found broken.","E/R - Aux. Engine,E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","New pipe fabriacted & installed. A new support bracket also fabricated & installed.","2022-08-22T23:59:35","NA","Completed","2022-05-22T23:59:35","No","No","No","Internal"]
[null,null,null,26052,95202,"0_Thu Jun 23 2022 17:22:32 GMT+0800","2022-05-25T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Galley AC Motor V-belt found brittle & damaged.","Accommodation","General Appearance","Equipment Related","10.32","Very High","","","V-Belt renewed with new spare. Tried out & in use.","2022-08-25T23:59:35","NA","Completed","2022-05-25T23:59:35","No","No","No","Internal"]
[null,null,null,26070,37004,"24_Tue Jun 28 2022 21:23:38 GMT+0800","2022-05-25T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Port side Gangway Air Motor not working.","Deck - Machinery","General Appearance","Equipment Related","5.47","Medium","","","Air Motor opened up for inspection. Found the air vanes damaged. Same renewed with new spare. Motor installed & tried out. In use.","2022-08-25T23:59:35","NA","Completed","2022-06-18T23:59:35","No","No","No","Internal"]
[null,null,null,26049,36613,"0_Thu Jun 23 2022 17:14:18 GMT+0800","2022-05-26T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Steering Gear Ram Drip Trays found secured by wire lashing.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","New quick release lashing fabricated & installed. Drip trays can now be removed easily, cleaned & then installed back.","2022-08-26T23:59:35","NA","Completed","2022-05-28T23:59:35","No","No","No","Internal"]
[null,null,null,26050,60995,"24_Thu Jun 23 2022 17:17:09 GMT+0800","2022-05-26T23:59:35","Observation","Ship Staff","Ship Staff Insp.","AE #1 Unit #4 & #6 Fuel Pump Return Line Flange found leaking slightly.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Flange gaskets renewed with new. ","2022-08-26T23:59:35","NA","Completed","2022-05-26T23:59:35","No","No","No","Internal"]
[null,null,null,26053,67267,"0_Thu Jun 23 2022 17:25:14 GMT+0800","2022-05-29T23:59:35","Observation","Ship Staff","Ship Staff Insp.","During Discharging, the Main Sea Water line pressure found reduced resulting in tripping of the Inert Gas Plant.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","External Factors","10.32","Very High","","","High Sea Chest Filter found completely choked with fish. Same cleaned/cleared.","2022-08-29T23:59:35","NA","Completed","2022-05-29T23:59:35","No","No","No","Internal"]
[null,null,null,26034,73651,"24_Fri Jun 24 2022 15:21:52 GMT+0800","2022-05-30T23:59:35","Observation","Ship Staff","Ship Staff Insp.","COP #2 Discharge Pressure Gauge showing incorrect readings.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.12","Medium","","","Renewed from spare.","2022-08-30T23:59:35","RO DBAU220130","Completed","2022-08-23T23:59:35","No","No","No","Internal",""]
[null,null,null,26054,67047,"0_Thu Jun 23 2022 17:27:52 GMT+0800","2022-05-30T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Deck Water Service Pump Discharge Line found leaking in the Steering Flat.","Deck - Machinery","General Appearance","Equipment Related","10.32","Very High","","","Pipeline section removed & repaired in the Workshop. Same installed back & pump tried out. Found in order.","2022-08-28T23:59:35","NA","Completed","2022-05-31T23:59:35","No","No","No","Internal"]
[null,null,null,26056,83191,"0_Thu Jun 23 2022 17:38:36 GMT+0800","2022-05-30T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Steering Gear Grease Pump found not operating satisfactorily.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Grease Pump timer & circuit wires found deteriorated. Same renewed with new. tried out & in order.","2022-08-30T23:59:35","NA","Completed","2022-06-03T23:59:35","No","No","No","Internal"]
[null,null,null,26055,15709,"0_Thu Jun 23 2022 17:34:18 GMT+0800","2022-06-01T23:59:35","Observation","Ship Staff","Ship Staff Insp.","ME Control Air Dryer Timer Panel Box found broken.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Renewed with new box. Fixing plate fabricated to install the box.","2022-09-02T23:59:35","NA","Completed","2022-06-02T23:59:35","No","No","No","Internal"]
[null,null,null,26061,38169,"24_Thu Jun 23 2022 17:31:01 GMT+0800","2022-06-01T23:59:35","Observation","Ship Staff","Ship Staff Insp.","EGB Soot Tank found unable to empty/pump out completely.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Soot Tank Line near Overboard valve found choked. Same opened up & cleared manually. installed back & tried out. Tank Emptied & cleaned.","2022-09-01T23:59:35","NA","Completed","2022-06-09T23:59:35","No","No","No","Internal"]
[null,null,null,26033,13609,"0_Thu Jun 23 2022 17:56:03 GMT+0800","2022-06-03T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Fire Alarm System showing Fault Smoke Sensor #22 Dirty.  After sensor renewal, fault showing \"Loop 1 Smoke 22 Present Not Configured – Fault(152)\"","LSA / FFA","Eng. / Strg. Comp.","Equipment Related","5.39","Very High","","","Smoke Sensor #22 – Incinerator Area was giving “Sensor Dirty” Fault.\nThe sensor was cleaned & installed back & the alarm was reset.\nAfter a few days, this alarm was again actuated. The sensor was cleaned & put back, but the alarm kept occuring frequently.\nThe sensor was renewed with a new sensor. The same has been added in the circuit as perthe manual procedure.\nNow, the system is showing “Loop 1 Smoke 22 Present Not Configured – Fault(152)”.\nTried to configure the system as per the onboard manual procedure menu 6. All alarms are now reset after uploading the config file & adding the missing sensors.","2022-09-03T23:59:35","NA","Completed","2022-07-02T23:59:35","No","No","No","Internal"]
[null,null,null,26057,70436,"0_Thu Jun 23 2022 17:40:34 GMT+0800","2022-06-04T23:59:35","Observation","Ship Staff","Ship Staff Insp.","ME Unit #2 Fuel Valve Aft found leaking by way of the return line banjo bolt.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Banjo bolt gaskets renewed with new spares.","2022-09-04T23:59:35","NA","Completed","2022-06-04T23:59:35","No","No","No","Internal"]
[null,null,null,26058,67438,"0_Thu Jun 23 2022 17:42:15 GMT+0800","2022-06-04T23:59:35","Observation","Ship Staff","Ship Staff Insp.","ME Unit #5 Exhaust Valve LO High Pressure Pipe leaking.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","HP Pipe renewed with onboard new spare.","2022-09-04T23:59:35","NA","Completed","2022-06-04T23:59:35","No","No","No","Internal"]
[null,null,null,26063,93821,"24_Fri Jun 24 2022 20:42:17 GMT+0800","2022-06-05T23:59:35","Observation","Ship Staff","Ship Staff Insp.","HFO Bunker Tank #1 Stbd bad quality bunker to be De-bunkered & Tank to be manually cleaned.","Hull & Tanks,E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","External Factors","","","","","Tank manually cleaned by shipstaff. Quantity of oil transferred to the waste oil tank is 0.8m3. Approximately 19~20 bags of sludge removed. There was some rust also accumulated on the first platform. This has been manually scraped & removed. The steam coils/lines have been checked & found in order. All rags/tools/equipment has been removed & the tank manholes have been secured.\n","2022-09-05T23:59:35","NA","Completed","2022-06-12T23:59:35","No","No","No","Internal"]
[null,null,null,26060,64591,"0_Thu Jun 23 2022 18:05:07 GMT+0800","2022-06-06T23:59:35","Observation","Ship Staff","Ship Staff Insp.","ME Jacket Cooling Water Pump #1 Found not on Stby.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Starter Module found defective. Same renewed with new onboard spare. Tried out & in order.","2022-09-06T23:59:35","NA","Completed","2022-06-06T23:59:35","No","No","No","Internal"]
[null,null,null,26035,96122,"0_Fri Jun 24 2022 15:27:49 GMT+0800","2022-06-08T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Elevator D-Deck Door not operational.","Accommodation","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","During inspection found working satisfactorily. No fault reported .","2022-09-08T23:59:35","RO DBAU220047","Completed","2022-08-27T23:59:35","No","No","No","Internal"]
[null,null,null,26059,98287,"0_Thu Jun 23 2022 17:47:13 GMT+0800","2022-06-08T23:59:35","Observation","Ship Staff","Ship Staff Insp.","VRCS return found damaged & leaking in two pipe sections.","Deck - Machinery,Deck - Pipe / Fittings","","Equipment Related","8.8","Medium","","","Pipe section removed & brought to ER Workshop. Renewed with new pipes. Installed & tried out.","2022-09-08T23:59:35","NA","Completed","2022-06-08T23:59:35","No","No","No","Internal"]
[null,null,null,26064,98540,"0_Fri Jun 24 2022 20:50:27 GMT+0800","2022-06-08T23:59:35","Observation","Ship Staff","Ship Staff Insp.","EGCS CO2 Gas Analyser readings for CO2 not matching on the LCRP & ECRP.\n","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Troubleshooting advised by maker is to \"Clear the Logbook\" for CO2 Analyser unit. Same carried out & readings matching now. System running satisfactorily.","2022-09-08T23:59:35","NA","Completed","2022-06-13T23:59:35","No","No","No","Internal"]
[null,null,null,28103,45621,"24_Tue Dec 27 2022 15:00:10 GMT+0800","2022-06-09T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Anchor washing line for both Port and starboard anchors was found damaged and holed. Pipelines to be renewed. ","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","Equipment Related","10.32","Very High","","","Total 5 pipe section removed for repairs/fabrication. Port side main manifold fabricated new and fitted. Repaired 4 branch pipe sections.","2022-07-08T23:59:35","","Completed","2023-02-01T23:59:35","No","No","No","Internal"]
[null,null,null,28104,45035,"0_Tue Dec 27 2022 15:03:34 GMT+0800","2022-06-09T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Crew change locker needs to be cleaned and arranged.","Accommodation","General Appearance","Behaviour Based","","","","","Crew change locker cleaned and arranged, and loose items removed.  \nDirty locker door Painted. ","2022-06-16T23:59:35","","Completed","2022-06-15T23:59:35","No","No","No","Internal"]
[null,null,null,28105,82434,"24_Tue Dec 27 2022 14:54:11 GMT+0800","2022-06-09T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Bunker line condition on deck iwo the pump room has a lot of rust spots. De-rusting and if the condition is bad then line renewal must be carried out.","Deck - Pipe / Fittings","General Appearance","Equipment Related","10.32","Very High","","","Bunker line  on deck deck in front of  the pump room has been de rusted and painted.","2022-07-08T23:59:35","","Completed","2022-12-17T23:59:35","No","No","No","Internal"]
[null,null,null,28106,70866,"24_Thu Dec 29 2022 11:44:47 GMT+0800","2022-06-09T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ECR AC pressure gauges were found damaged. Same to be renewed. ","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Renewed from spare.","2022-07-10T23:59:35","","Completed","2022-08-30T23:59:35","No","No","No","Internal"]
[null,null,null,28107,80408,"24_Thu Dec 29 2022 11:39:45 GMT+0800","2022-06-09T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Damaged fire sensor in the Pump room to be renewed","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.39","Very High","","","Renewed from spare","2022-06-17T23:59:35","","Completed","2022-08-13T23:59:35","No","No","No","Internal"]
[null,null,null,28108,49637,"24_Thu Dec 29 2022 11:51:51 GMT+0800","2022-06-09T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","DO line butterfly valve iwo the Pump room for the drip sampler was found jammed. To be freed up","Deck - Pipe / Fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Valve eased up for proper operation, Sampler removed from place and blank flange placed.","2022-07-10T23:59:35","","Completed","2022-12-28T23:59:35","No","No","No","Internal"]
[null,null,null,28109,78443,"24_Thu Dec 29 2022 11:47:06 GMT+0800","2022-06-09T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Damaged U bolt for ME JW outlet line. ","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Renewed from spare","2022-06-24T23:59:35","","Completed","2022-06-23T23:59:35","No","No","No","Internal"]
[null,null,null,26062,39750,"24_Fri Jun 24 2022 20:37:24 GMT+0800","2022-06-10T23:59:35","Observation","Ship Staff","Ship Staff Insp.","VRCS Return line found holed & leaking. ","Deck - Pipe / Fittings,Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","LIne section removed & brought to ER Workshop. Same renewed with new fabricated pipe. Installed, tried out & found in order.","2022-09-10T23:59:35","NA","Completed","2022-06-10T23:59:35","No","No","No","Internal"]
[null,null,null,26065,55447,"24_Fri Jun 24 2022 20:45:28 GMT+0800","2022-06-11T23:59:35","Critical Equipment,Observation","Ship Staff","Ship Staff Insp.","Steering Gear #1 Servo Motor found with slight noise/vibration.","Critical Equip.,Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Motor removed to inspection. The spider coupling was found completely worn out/broken. Spider coupling replaced with new spare. The motor was renewed with new spare onboard.","2022-09-12T23:59:35","NA","Completed","2022-06-12T23:59:35","No","No","No","Internal"]
[null,null,null,26036,63409,"24_Fri Jun 24 2022 20:56:54 GMT+0800","2022-06-12T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Elevator Breaker Switch No. 2 found tripping.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Presently working satisfactorily during inspection and no fault reported.\n","2022-09-12T23:59:35","RO DBAU220047","Completed","2022-08-27T23:59:35","No","No","No","Internal"]
[null,null,null,26069,86360,"24_Tue Jun 28 2022 13:26:16 GMT+0800","2022-06-12T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Stern Flag Pole Hoisting Pulley found wasted/broken.","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.4","Very High","","","Flag pole removed & brought to the ER Workshop. A new pulley arrangement fabricated & welding. Flag Pole installed.","2022-09-12T23:59:35","NA","Completed","2022-06-15T23:59:35","No","No","No","Internal"]
[null,null,null,26037,97508,"24_Fri Jun 24 2022 20:59:25 GMT+0800","2022-06-13T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Elevator Engine Room E1 Door interlock switch & magnetic switch malfunctioning frequently.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Need to renew the magnetic switches & interlock switches as they are worn out due to age. RO raised. Presently found working during inspection.","2022-09-13T23:59:35","RO DBAU220047","Completed","2022-08-27T23:59:35","No","No","No","Internal"]
[null,null,null,26066,73105,"0_Fri Jun 24 2022 20:53:25 GMT+0800","2022-06-13T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Sewage Vacuum System found not working in several cabins & common spaces.","E/R - Pipes/ valves & fittings","MLC Related","Inappropriate Procedure","10.32","Very High","","","One complete section of the sewage system found choked with large quantity of tissue/toilet paper. Pipe section removed & manually cleared. Installed back & tried out. System back in use.","2022-09-13T23:59:35","NA","Completed","2022-06-14T23:59:35","No","No","No","Internal"]
[null,null,null,26040,39532,"24_Tue Jun 28 2022 12:49:56 GMT+0800","2022-06-15T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Elevator & Auto-Telephone found not working.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Renewed telephone, tried out found working satisfactorily.","2022-09-15T23:59:35","RO DBAU220084","Completed","2022-09-19T23:59:35","No","No","No","Internal"]
[null,null,null,26041,35874,"24_Tue Jun 28 2022 12:56:50 GMT+0800","2022-06-15T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Sound Powered Telephone in ECR found not working. Keypads/push buttons for various phones not working & damaged due to ageing. ","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","new generator installed,  Working satisfactorily.","2022-09-15T23:59:35","RO DBAU220105","Completed","2022-08-28T23:59:35","No","No","No","Internal"]
[null,null,null,26042,95985,"24_Tue Jun 28 2022 12:58:47 GMT+0800","2022-06-15T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Sound Powered phone Headsets for Emcy Maneuvering, Steering Gear & COP Platform found not working.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Renewed and working satisfactorily.","2022-09-15T23:59:35","RO DBAU220105","Completed","2022-08-22T23:59:35","No","No","No","Internal"]
[null,null,null,26044,30365,"24_Tue Jun 28 2022 21:18:18 GMT+0800","2022-06-16T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Deck Foam Line Isolation Valve #4, #5 & #6 found not holding during routine trying out.","LSA / FFA,Deck - Pipe / Fittings","Safety / LSA / FFA","Equipment Related","","","","","No6 Foam isolation valve renewed.  4 & 5 Freed.","2022-09-16T23:59:35","RO DBAU220137","Completed","2022-10-02T23:59:35","No","No","No","Internal"]
[null,null,null,26043,80285,"24_Tue Jun 28 2022 21:14:13 GMT+0800","2022-06-17T23:59:35","Observation","Ship Staff","Ship Staff Insp.","SSAS Alarm malfunctioning & getting activated frequently.","Navigation - Others","ISPS Related","Equipment Related","7.6","Medium","","","Suspect the SSAS unit is faulty. The push buttons have been disconnected & the unit has been switched to \"OFF\" position. Complete SSAS unit along with wiring renewed with onboard new spare. Tried out & found in order.","2022-09-17T23:59:35","NA","Completed","2022-07-02T23:59:35","No","No","No","Internal"]
[null,null,null,26045,72732,"24_Wed Jun 29 2022 16:40:21 GMT+0800","2022-06-18T23:59:35","Observation","Ship Staff","Ship Staff Insp.","AE #1 Fuel Oil Differential Pressure Sensor found defective.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Renewed and found working satisfactory.","2022-09-18T23:59:35","RO DBAU220133","Completed","2022-08-14T23:59:35","No","No","No","Internal","Spare will be supplied at first convenient port. Renew the same once it is received."]
[null,null,null,26068,56207,"24_Tue Jun 28 2022 13:18:43 GMT+0800","2022-06-18T23:59:35","Observation","Ship Staff","Ship Staff Insp.","ME Unit #3 Stuffing Box Top Scraper Ring Spring found broken during routine Under piston Cleaning.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","The old broken spring sections removed. A new spring was installed in place. ","2022-09-18T23:59:35","NA","Completed","2022-06-18T23:59:35","No","No","No","Internal"]
[null,null,null,26460,63738,"24_Sat Jul 16 2022 09:47:16 GMT+0800","2022-06-20T23:59:35","Observation","Ship Staff","Ship Staff Insp.","BWTS Mimic panel frozen without any alarm during De-ballasting operations at Loadport.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","6.21","High","","","Checked by visiting techinican found all in order during his stay.","2022-09-20T23:59:35","","Completed","2022-09-16T23:59:35","No","No","No","Internal"]
[null,null,null,29545,23912,"24_Tue Mar 14 2023 14:15:17 GMT+0800","2022-06-20T23:59:35","Observation","Ship Staff","Nav Audit / Verification","Inmarsat c- no. 2 antenna transmission - non functional- Previous observation not rectified  ","Navigation - GMDSS & Communication","","Knowledge Based","4.23","High","","","Monthly / weekly test of GMDSS equipment must be carried out diligently and finding must be reported/ rectified on priority basis.\nSpecial attention must paid to SAT-C transmitter and Receiver unit is working properly or not. Same to be recorded in GMDSS log book \n","2022-09-19T23:59:35","","Completed","2022-06-24T23:59:35","No","No","No","Internal"]
[null,null,null,29546,23322,"0_Tue Mar 14 2023 14:21:14 GMT+0800","2022-06-20T23:59:35","Observation","Ship Staff","Nav Audit / Verification","M.E RPM indicator marking are faded on STBD side bridge wing","Navigation - Others","Navigation","Knowledge Based","4.7","High","","","Astern marking on STBD bridge wing RPM indicator carried out.","2022-09-19T23:59:35","","Completed","2022-07-03T23:59:35","No","No","No","Internal"]
[null,null,null,29547,79901,"0_Tue Mar 14 2023 14:22:43 GMT+0800","2022-06-20T23:59:35","Observation","Ship Staff","Nav Audit / Verification","Navtex antenna earthing wire on monkey island is broken ","Navigation - GMDSS & Communication","Navigation","Knowledge Based","4.7","High","","","Earthing wire renewed for Navtex antenna. All other antenna earthing  wire inspected on Monkey Island for any damage.","2022-09-19T23:59:35","","Completed","2022-07-03T23:59:35","No","No","No","Internal"]
[null,null,null,29548,36221,"0_Tue Mar 14 2023 14:24:11 GMT+0800","2022-06-20T23:59:35","Observation","Ship Staff","Nav Audit / Verification","No1 VHF / RT antenna needs bracket fabrication(Broken).  ","Navigation - GMDSS & Communication","Navigation","Knowledge Based","4.7","High","","","No1 VHF / RT antenna was fabricated with permanent arrangement.","2022-09-19T23:59:35","","Completed","2022-07-01T23:59:35","No","No","No","Internal"]
[null,null,null,29549,72034,"0_Tue Mar 14 2023 14:26:22 GMT+0800","2022-06-20T23:59:35","Observation","Ship Staff","Nav Audit / Verification","Main mast air horn not working properly    ","Navigation - Others","Navigation","Behaviour Based","4.7","High","","","Draining of main mast air horn line was carried out to removed any condense water from the line.\nDiaphragm and solenoid valve was cleaned and put back. \nWhistle tried out several time working satisfactory.  \n","2022-09-19T23:59:35","","Completed","2022-07-08T23:59:35","No","No","No","Internal"]
[null,null,null,29550,31482,"0_Tue Mar 14 2023 14:28:33 GMT+0800","2022-06-20T23:59:35","Observation","Ship Staff","Nav Audit / Verification","Water leaking in Nav locker on top of  main GYRO unit (Wire coming to Nav locker from monkey island sealing is not proper)     ","Navigation - Others","Navigation","Behaviour Based","4.7","High","","","Silicone applied at that area and water leaking was stopped . ","2022-09-19T23:59:35","","Completed","2022-07-03T23:59:35","No","No","No","Internal"]
[null,null,null,29551,36018,"0_Tue Mar 14 2023 14:29:51 GMT+0800","2022-06-20T23:59:35","Observation","Ship Staff","Nav Audit / Verification","Main mast air horn drain valve wheel is broken difficult to operate valve.     ","Navigation - Others","Navigation","Equipment Related","4.7","High","","","Darin valve wheel was  replaced with new wheel    ","2022-09-19T23:59:35","","Completed","2022-07-01T23:59:35","No","No","No","Internal"]
[null,null,null,29552,31870,"0_Tue Mar 14 2023 14:32:09 GMT+0800","2022-06-20T23:59:35","Observation","Ship Staff","Nav Audit / Verification","BNWAS was in default password","Navigation - Others","Navigation","Behaviour Based","4.7","High","","","BNWAS password change at the same time and put in Manual mode ","2022-09-19T23:59:35","","Completed","2022-06-21T23:59:35","No","No","No","Internal"]
[null,null,null,29553,95664,"0_Tue Mar 14 2023 14:33:49 GMT+0800","2022-06-20T23:59:35","Observation","Ship Staff","Nav Audit / Verification","MF/HF access door hinges are broken.    ","Navigation - GMDSS & Communication","Navigation","Knowledge Based","4.7","High","","","MF/HF access door taken to E/R workshop for rectification. Same door fit back after rectification. ","2022-09-19T23:59:35","","Completed","2022-08-02T23:59:35","No","No","No","Internal"]
[null,null,null,29554,76770,"0_Tue Mar 14 2023 14:18:58 GMT+0800","2022-06-20T23:59:35","Observation","Ship Staff","Nav Audit / Verification","Bridge clock second's needle not operational","Navigation - Others","Navigation","Knowledge Based","4.7","High","","","Bridge clock second needle was stuck on glass. Needle was made free by removing cover glass. \nClock is working satisfactory \n","2022-09-19T23:59:35","","Completed","2022-07-04T23:59:35","No","No","No","Internal"]
[null,null,null,29555,90950,"0_Tue Mar 14 2023 14:35:34 GMT+0800","2022-06-20T23:59:35","Observation","Ship Staff","Nav Audit / Verification","Anemometer showing wrong direction of wind (Almost 50 degree more to STBD)    ","Navigation - Others","Navigation","Equipment Related","4.7","High","","","Inspection of Anemometer carried out turning bearing was getting stuck at some direction.\nBearing was made free by applying grease and oil. Anemometer free to rotate on its axis working satisfactory. \n","2022-09-19T23:59:35","","Completed","2022-07-08T23:59:35","No","No","No","Internal"]
[null,null,null,26071,91582,"24_Thu Jun 30 2022 12:58:35 GMT+0800","2022-06-20T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Reefer Compressor #2 V-Belt found broken.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Only one v-belt found broken. All V-belts renewed. Will order the same in next store requisition.","2022-09-20T23:59:35","","Completed","2022-06-20T23:59:35","No","No","No","Internal","Vessel to raise RO and also check other refer compressor V belt."]
[null,null,null,26046,72680,"24_Fri Jul 01 2022 20:10:39 GMT+0800","2022-06-21T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Both Ballast Eductors Suction & Discharge Pressure gauge cocks found frozen in open position & not operable.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.80","Medium","","","Lines checked & cleared. Gauge cocks freed up.","2022-09-21T23:59:35","NA","Completed",null,"No","No","No","Internal"]
[null,null,null,26469,94413,"24_Sat Jul 16 2022 09:25:08 GMT+0800","2022-06-23T23:59:35","Observation","Ship Staff","Ship Staff Insp.","FW Tank (P) Outlet Line to Deck Service Pump found holed & leaking in two locations along the pipe seam.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Pipe could not be removed due to EGCS piping. Section cut & removed. Entire pipe section renewed with one addtional flanges set in order to install/remove in the future. Rectified.","2022-10-03T23:59:35","NA","Completed","2022-07-03T23:59:35","No","No","No","Internal"]
[null,null,null,26461,97110,"0_Fri Jul 15 2022 09:38:31 GMT+0800","2022-06-24T23:59:35","Observation","Ship Staff","Ship Staff Insp.","HFO Purifier #1 Bowl found leaking.","E/R - Purifier","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Bowl height checked & found to be 6mm less than required. Opened up the vertical shaft & found the flat spring broken. flat spring renewed. All Vertical shaft bearings also renewed. Purifier tried out & found in order.","2022-09-24T23:59:35","NA","Completed","2022-06-27T23:59:35","No","No","No","Internal"]
[null,null,null,26462,98128,"0_Fri Jul 15 2022 09:40:17 GMT+0800","2022-06-25T23:59:35","Observation","Ship Staff","Ship Staff Insp.","AE #2 Unit #6 Rocker Arm Coaming Cover leaking.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Coaming Cover & Gasket replaced with new spares. Tried out & leak recitified.","2022-09-25T23:59:35","NA","Completed","2022-06-25T23:59:35","No","No","No","Internal"]
[null,null,null,26463,85088,"24_Fri Jul 15 2022 09:41:54 GMT+0800","2022-06-25T23:59:35","Observation","Ship Staff","Ship Staff Insp.","AE #2 Oilmax Pump Seal leaking","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Pump overhauled & seal renewed. tried out & in use.","2022-09-25T23:59:35","NA","Completed","2022-06-25T23:59:35","No","No","No","Internal"]
[null,null,null,26464,49086,"24_Fri Jul 15 2022 09:44:37 GMT+0800","2022-06-26T23:59:35","Observation","Ship Staff","Ship Staff Insp.","ECR AC #1 Compressor giving low insulation & overheating.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","AC Compressor renewed with new spare. System charged with gas & tried out. Performance Satisfactory & in use.","2022-09-26T23:59:35","NA","Completed","2022-06-28T23:59:35","No","No","No","Internal"]
[null,null,null,26465,26727,"0_Fri Jul 15 2022 09:47:22 GMT+0800","2022-06-27T23:59:35","Observation","Ship Staff","Ship Staff Insp.","ER Floodlight for 2nd Deck Stbd Aft found not working.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Ignitor & Ballast found damaged. Floodlight renewed with new supplied LED floodlight. Tried out & in use.","2022-09-28T23:59:35","NA","Completed","2022-06-28T23:59:35","No","No","No","Internal"]
[null,null,null,26466,36003,"24_Sat Jul 16 2022 08:48:49 GMT+0800","2022-06-27T23:59:35","Observation","Ship Staff","Ship Staff Insp.","IG O2 Analyser Goose Neck Pipe rusted & worn out.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Pipe section renewed. Rectified.","2022-09-29T23:59:35","NA","Completed","2022-06-29T23:59:35","No","No","No","Internal"]
[null,null,null,26453,56471,"0_Fri Jul 15 2022 09:52:29 GMT+0800","2022-06-28T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Fwd Whistle found not working.","Navigation - Others","Navigation","Equipment Related","4.7","High","","","Spares available onboard and vessel will carry out the job.\nForward whistle replaced with new.  Tested and found working good.","2022-12-05T23:59:35","","Completed","2022-12-02T23:59:35","No","No","No","Internal","Has the vessel received the spares? What is the present condition?"]
[null,null,null,26470,94821,"24_Fri Jul 15 2022 09:59:21 GMT+0800","2022-06-28T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Aux. Boiler #2 Gauge Glass Stbd side leaking & discoloured.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Gauge Glass gaskets renewed. Leak rectified.","2022-09-29T23:59:35","NA","Completed","2022-06-29T23:59:35","No","No","No","Internal"]
[null,null,null,26467,85311,"0_Sat Jul 16 2022 08:55:07 GMT+0800","2022-06-30T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Deck Seal Pumps Discharge Line Distance piece leaking via pinhole.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Distance piece repaired. Installed & tried out. Rectified.","2022-10-02T23:59:35","NA","Completed","2022-07-02T23:59:35","No","No","No","Internal"]
[null,null,null,26459,68013,"24_Sat Jul 16 2022 09:40:20 GMT+0800","2022-07-01T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Fire Alarm System giving frequent alarms due to dirty/defective sensors.","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.35","Medium","","","Renewed from spare","2022-10-01T23:59:35","RO DBAU220131","Completed","2022-08-08T23:59:35","No","No","No","Internal"]
[null,null,null,26468,50363,"0_Sat Jul 16 2022 08:57:02 GMT+0800","2022-07-01T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Cascade Tank Steam Inlet Y-Filter leaking via Drain Plug.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Drain Plug gasket renewed. Leak Rectified.","2022-10-02T23:59:35","NA","Completed","2022-07-02T23:59:35","No","No","No","Internal"]
[null,null,null,26454,53276,"0_Sat Jul 16 2022 08:51:20 GMT+0800","2022-07-02T23:59:35","Observation","Ship Staff","Ship Staff Insp.","AE #3 Oilmax Discharge Hose found leaking.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Renewed the hose and rectified the leaks","2022-12-01T23:59:35","DBAU220196","Completed","2022-11-02T23:59:35","No","No","No","Internal"]
[null,null,null,26458,76523,"24_Sat Jul 16 2022 11:28:07 GMT+0800","2022-07-02T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Main Fuel Oil Circulating Pump #1 Spider Coupling found damaged.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Renewed spider coupling","2022-10-02T23:59:35","RO DBAU220145","Completed","2022-08-09T23:59:35","No","No","No","Internal"]
[null,null,null,26455,33300,"24_Sat Jul 16 2022 09:56:41 GMT+0800","2022-07-06T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Incinerator Combustion Chamber Thermocouple Damaged.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Tried out found working satisfactorily.","2022-10-06T23:59:35","RO DBAU220152","Completed","2022-08-27T23:59:35","No","No","No","Internal","Spare has been supplied. Please renew the thermocouple and try out the Incinerator."]
[null,null,null,26456,56233,"24_Sat Jul 16 2022 11:22:02 GMT+0800","2022-07-06T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Main Fuel Oil Circulating Pump #1 mechanical Seal leaking","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Overhauled and arrested the leaks","2022-10-06T23:59:35","RO DBAU220096","Completed","2022-08-09T23:59:35","No","No","No","Internal"]
[null,null,null,26457,12988,"24_Sat Jul 16 2022 11:22:32 GMT+0800","2022-07-07T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Immersion Suits (7 pieces) found damaged.","LSA / FFA","Safety / LSA / FFA","","5.33","High","","","RO to be raised.","2022-10-07T23:59:35","Requisition received and damaged suits replaced.","Completed","2022-08-04T23:59:35","No","No","No","Internal","RO needs to be raised and then it will be supplied by the office."]
[null,null,null,27462,22390,"0_Thu Aug 11 2022 14:16:13 GMT+0800","2022-07-12T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Accomodation Gas Detection System AHU #1 Gas Sensor Defective.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","Sensor renewed,, working satisfactory","2022-10-12T23:59:35","RO DBAU220157","Completed","2023-01-28T23:59:35","No","No","No","Internal","AWAITING READINESS \nESTIMATED READINESS DATE : 17/10/2022"]
[null,null,null,27465,93715,"0_Thu Aug 11 2022 14:12:53 GMT+0800","2022-07-17T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Steering Gear #2 Coupling Chain Cover found with no grease.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Presently no leaks","2022-10-17T23:59:35","","Completed","2022-07-17T23:59:35","No","No","No","Internal"]
[null,null,null,27466,10324,"24_Thu Aug 11 2022 14:22:26 GMT+0800","2022-07-18T23:59:35","Observation","Ship Staff","Ship Staff Insp.","ME FO Circulating Pump #2 Mechanical Seal Leaking.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Renewed the seal and presently no leaks","2022-10-18T23:59:35","RO DBAU220145","Completed","2022-07-18T23:59:35","No","No","No","Internal"]
[null,null,null,27463,35453,"24_Thu Aug 11 2022 13:57:13 GMT+0800","2022-07-23T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Aft Hydraulic Winch (Port) leaked during berthing Zhoushan.","Deck - Mooring Machinery","Mooring","Equipment Related","","","","","Mooring winch M10, speed control valve block and counter balance valve block cover renewed by GMTS technicians at Fujairah on 10.Feb.2023 using spares on board. After renewal purging of the system carried out and tested for operation and leaks. Mooring winch working satisfactory with no leaks.","2022-10-23T23:59:35","RO DBAU220169","Completed","2023-02-08T23:59:35","No","No","No","Internal","Spare block was found in the store and was renewed. Please confirm same."]
[null,null,null,27467,74546,"0_Thu Aug 11 2022 14:01:15 GMT+0800","2022-07-23T23:59:35","Observation","Ship Staff","Ship Staff Insp.","ME found unable to increase rpm beyond 54rpm","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Due to less viscous LSMGO M/E is not able to increase as the air fuel ratio is set for HSFO, The Nabtesco program has to be modified to carryout the change. Presently using higher viscous LSMGO and found the raise in rpm to be gradual.","2022-10-23T23:59:35","","Completed","2022-08-19T23:59:35","No","No","No","Internal"]
[null,null,null,27470,30785,"0_Thu Aug 11 2022 14:04:05 GMT+0800","2022-07-23T23:59:35","Observation","Others (Eg. Insurance etc.)","Others (Eg. Insurance etc.)","ME unable to fire on Astern Kick during Arrival Zhoushan Berth.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Investigated by Techinicians ashore and observed the cause to be less viscous LSMGO, To install chiller in the fuel line and to use higher viscosity bunker.","2022-10-23T23:59:35","","Completed","2022-08-04T23:59:35","No","No","No","External"]
[null,null,null,27514,94995,"0_Thu Aug 11 2022 14:28:26 GMT+0800","2022-07-26T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Main Air Bottle #2 Pressure Transmitter defective.","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","New transmitter renewed and found working satisfactorily.","2022-10-26T23:59:35","DBAU220178","Completed","2022-10-28T23:59:35","No","No","No","Internal","Order placed and delivery will be End of October"]
[null,null,null,27468,80174,"24_Thu Aug 11 2022 14:09:35 GMT+0800","2022-07-27T23:59:35","Observation","Ship Staff","Ship Staff Insp.","AE #2 Fuel Oil Differential Pressure Sensor found defective","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","renewed from spare","2022-10-27T23:59:35","RO DBAU220133","Completed","2022-08-23T23:59:35","No","No","No","Internal"]
[null,null,null,27469,28653,"0_Thu Aug 11 2022 14:06:38 GMT+0800","2022-07-28T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Accom. AC Compressor #1 Shaft Seal Leaking.","Accommodation","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Shaft seal replaced with new spare. Gas recharged in the system & tried out. In order. RO to be raised for spare shaft seal. ","2022-10-28T23:59:35","","Completed",null,"No","No","No","Internal"]
[null,null,null,27458,64264,"24_Fri Sep 02 2022 23:35:26 GMT+0800","2022-07-31T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Steering gear exhaust fan blades are damaged","Deck - Machinery","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Steering gear exhaust fan renewed","2022-10-30T23:59:35","DBAU220183","Completed","2023-01-18T23:59:35","No","No","No","Internal","Order will be ready by end of October."]
[null,null,null,27459,28098,"0_Fri Sep 02 2022 20:52:15 GMT+0800","2022-08-05T23:59:35","Observation","Ship Staff","Ship Staff Insp.","No dedicated lifting davit provided for lifting small bunker hoses (Lub oIl) on Port and stbd ship side main deck in front of  break of accommodation.","Deck - Machinery","ISM Related","Industry Issue,Equipment Related","8.50","Medium","","","Deferred to dry dock and REFMAN specs raised.","2022-11-05T23:59:35","","Completed","2022-11-24T23:59:35","No","No","No","Internal","Please enter this in REFMAN and then close this item from DDRL."]
[null,null,null,27480,58202,"24_Fri Sep 02 2022 20:25:07 GMT+0800","2022-08-08T23:59:35","Critical Equipment","Ship Staff","Ship Staff Insp.","Dedicated class approved Loadicator  hanging off, and not  operating.","Critical Equip.","Cargo / Ballast Systems","Equipment Related","8.4","Medium","","","New Loadicator with Load com Program Version 2.0 received at Singapore.  Checked function with Loadicator Test condition.  Found same as required.  ","2022-09-12T23:59:35","DBAU 225056","Completed","2022-09-16T23:59:35","No","No","No","Internal","Version 2.0 has been supplied. Flag has been notified. Now we need to carry out Class survey to closure. Loadicator is working fine."]
[null,null,null,27476,40914,"24_Fri Sep 02 2022 23:27:26 GMT+0800","2022-08-09T23:59:35","Observation","Ship Staff","Others (Eg. Insurance etc.)","Insulation gloves for MSB and ESB more than two years old.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.24","Low","","","Renewed the gloves","2022-11-08T23:59:35","DBAU220182","Completed","2022-09-17T23:59:35","No","No","No","Internal","RO has been raised and items supplied. Please confirm."]
[null,null,null,27513,62388,"24_Fri Sep 02 2022 23:22:12 GMT+0800","2022-08-09T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Meat room door sealing is brittle due to overheating","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Renewed the gasket from spare received at singapore on 01/11/22. Found working satisfactorily.","2022-11-08T23:59:35","DBAU220180","Completed","2022-11-01T23:59:35","No","No","No","Internal","Item should have been supplied In singapore. \nPlease check"]
[null,null,null,28289,26918,"0_Sun Jan 08 2023 10:14:21 GMT+0800","2022-08-09T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Port Pump room blower drain pipe found holed. Needs to be renewed. ","Deck - Machinery","Structural Condn. / WT integrity ","Equipment Related","10.32","Very High","","","Drain Pipe wasted section renewed.","2022-09-08T23:59:35","","Completed","2023-01-11T23:59:35","No","No","No","Internal"]
[null,null,null,28290,56719,"24_Sun Jan 08 2023 10:18:36 GMT+0800","2022-08-09T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Port Hose Handling Crane local starting panel door hinge found broken. Needs to be repaired. ","Cargo Mach.","Structural Condn. / WT integrity ","Equipment Related","8.63","High","","","Port Hose Handling Crane local starting panel door hinges repaired and fitted.","2022-09-09T23:59:35","","Completed","2023-01-11T23:59:35","No","No","No","Internal"]
[null,null,null,28291,54294,"24_Sun Jan 08 2023 10:21:41 GMT+0800","2022-08-09T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Welding burn marks were noted in the High Expansion Foam Room bulkhead. Needs to be painted. ","Miscellaneous","General Appearance","External Factors","8.63","High","","","Welding burn marks on High Expansion Foam Room bulkhead covered using paint.","2023-11-08T23:59:35","","Completed","2023-01-11T23:59:35","No","No","No","Internal"]
[null,null,null,28293,23451,"24_Sun Jan 08 2023 09:59:11 GMT+0800","2022-08-09T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Fire patrol plan on the bridge is not approved by the office. ","","ISM Related","Inappropriate Procedure","4.4","High","","","Approved Fire round plan received from office.","2022-08-24T23:59:35","","Completed","2023-01-09T23:59:35","No","No","No","Internal"]
[null,null,null,28296,73722,"24_Sun Jan 08 2023 10:07:06 GMT+0800","2022-08-09T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Chargers for Personnel Gas meters in the CCR are properly secured and susceptible to damage. ","Accommodation,Critical Equip.","Safety / LSA / FFA","Equipment Related","5.23","Very High","","","Chargers for Personnel Gas meters in the CCR  secured","2022-08-24T23:59:35","","Completed","2022-08-23T23:59:35","No","No","No","Internal"]
[null,null,null,28297,93333,"24_Sun Jan 08 2023 10:10:57 GMT+0800","2022-08-09T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","The cosmetic condition and cleanliness of the Fore peak store need to be upgraded. ","Miscellaneous","General Appearance","External Factors","11.12","Low","","","Cleaning of fore peak store carried out and Store Arranged.","2022-08-24T23:59:35","","Completed","2022-08-24T23:59:35","No","No","No","Internal"]
[null,null,null,28298,23107,"24_Sat Jan 14 2023 12:08:05 GMT+0800","2022-08-09T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Junction box Starboard side bridge wing is not permanently secured","Elect. Mach. & Equip.","General Appearance","Behaviour Based","10.37","Medium","","","Secured properly.","2023-08-19T23:59:35","","Completed","2023-01-09T23:59:35","No","No","No","Internal"]
[null,null,null,28299,22506,"24_Sat Jan 14 2023 13:20:41 GMT+0800","2022-08-09T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Oil leak was noted on the Alpha lubricator LO. tank","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","No.1 pump renewed from spare, Arrested all leaks by tightening the flanges.","2022-08-16T23:59:35","","Completed","2022-11-14T23:59:35","No","No","No","Internal"]
[null,null,null,28300,78281,"24_Sat Jan 14 2023 13:29:44 GMT+0800","2022-08-09T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","M/E Spare starting air valve found with rust marks.","E/R - Main Engine","General Appearance","Human Error","10.32","Very High","","","Buffed and cleaned the valve, parked it properly.","2022-09-09T23:59:35","","Completed","2023-01-05T23:59:35","No","No","No","Internal"]
[null,null,null,28301,12497,"24_Sat Jan 14 2023 12:18:13 GMT+0800","2022-08-09T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Excess dust and grease accumulation were found on Quick closing valve springs.","E/R - Pipes/ valves & fittings","General Appearance","External Factors","10.32","Very High","","","Cleaned and removed the dust.","2022-08-23T23:59:35","","Completed","2023-01-03T23:59:35","No","No","No","Internal"]
[null,null,null,28302,36438,"24_Sat Jan 14 2023 13:27:07 GMT+0800","2022-08-09T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","LSMGO Sample point inbetween pump room needs to be derusted, butterfly valve needs to be eased up.","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","External Factors","6.8","High","","","Derusted the line and eased up the valve.","2022-09-09T23:59:35","","Completed","2023-01-10T23:59:35","No","No","No","Internal"]
[null,null,null,27477,25231,"24_Fri Sep 02 2022 23:33:07 GMT+0800","2022-08-16T23:59:35","Defect","Ship Staff","Others (Eg. Insurance etc.)","Fire detection system is having fault of Repeater unit and battery failure alarm","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.35","Medium","","","Renewed the spares","2022-11-15T23:59:35","DBAU225058","Completed","2022-09-20T23:59:35","No","No","No","Internal","Engineering audit was not carried out in August. These items have been reported by ship staff. Please change the inspection type accordingly. Spare have been supplied under mentioned RO. Please confirm if the issue has been rectified or not."]
[null,null,null,27472,22130,"24_Fri Sep 02 2022 20:39:41 GMT+0800","2022-08-17T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Excessive spot rust found on boat deck, accommodation blocks, and tank domes, winches.","Deck - Machinery","General Appearance","Equipment Related","11.1","High","","","Hydro blaster to made fully operational.  Spares pending.\nHydroblaster spare nozzle and spare parts for nozzle received at Singapore on 23 Sept 2022.  Started hydroblasting  rusted area on deck.","2022-11-17T23:59:35","DBAU 220147","Completed","2022-09-21T23:59:35","No","No","No","Internal","Till the time hydro blaster spares are not supplied, carry out spot de-rusting and maintenance to be carried out. Send update in weekly work done report."]
[null,null,null,27473,31895,"24_Fri Sep 02 2022 20:32:21 GMT+0800","2022-08-17T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Steam smothering line from accommodation front to mast riser found rusted.  Need replacement.","Deck - Pipe / Fittings","Safety / LSA / FFA","Equipment Related","11.4","Very High","","","Pipes received, but 'U\" clamps and bolts not received.\n5 Section of Pipe renwed and U bolts received at Singapore on 23 Sept 2022.  All U bolts renewed.","2022-09-22T23:59:35","DBAU 220148","Completed","2022-09-21T23:59:35","No","No","No","Internal","U clamps have been supplied. Complete renewal should be completed during this voyage."]
[null,null,null,27478,19914,"24_Fri Sep 02 2022 19:07:50 GMT+0800","2022-08-17T23:59:35","Observation","Ship Staff","Engineering Audit","Port lifeboat engine found to raise and run ","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.27","Medium","","","Adjusted the tappet as per manual, Reduced the fuel setting and presently working satisfactorily.","2022-09-22T23:59:35","","Completed","2022-08-17T23:59:35","No","No","No","Internal"]
[null,null,null,27474,38875,"24_Fri Sep 02 2022 23:43:09 GMT+0800","2022-08-19T23:59:35","Defect","Ship Staff","Mooring Audit","STBD anchor windlass break spindle broken","Deck - Mooring Machinery","Eng. / Strg. Comp.","Equipment Related","9.20","Medium","","","Fabricated the broken piece and tried out found working satisfactorily. .","2022-11-18T23:59:35","DPEO220173","Completed","2022-08-29T23:59:35","No","No","No","Internal","This item not part of Mooring Audit. This was noted by Ship staff. Good work done by ship staff. This defect can be closed as same has been rectified. New spindle has been ordered and will be supplied during next SG call. PO DBAU225068 has been raised by office."]
[null,null,null,27456,68388,"24_Fri Sep 02 2022 22:21:56 GMT+0800","2022-08-20T23:59:35","Critical Equipment","Ship Staff","Ship Staff Insp.","No closed gas tight type cargo/ sampling and gas measuring equipment on board.  Requisition pending","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.12","Medium","","","Superintendent comments noted and observation closed.","2022-11-20T23:59:35","PO DBAU  220162 & DBAU 220176","Completed","2022-11-24T23:59:35","No","No","No","Internal","Ships action taken comment missing. \nThis defect to be closed as for pure tankers Closed type is not mandatory. Mail regarding same has been sent to the vessel. Vessel has restricted type UTI tape and same is acceptable as per OCIMF. DBAU220176 will be supplied."]
[null,null,null,27475,79304,"24_Fri Sep 02 2022 23:37:17 GMT+0800","2022-08-21T23:59:35","Critical Equipment","Ship Staff","Ship Staff Insp.","Gas sensors for 3 numbers of GX 2009 personal gas meters over due for renewal.  (2 oxygen sensors not working)  No spare sensors on board for any portable and Personal gas meters","Critical Equip.","Safety / LSA / FFA","Equipment Related","5.23","Very High","","","Date mentioning expiry of sensors and total inventory list  will be forwarded to Bruusgaurd company.  Requesting of replacement of expired sensors and additional spare sensors.\nNew sensors received for 3 Personal gas meters renewed on 24 Sept 2022","2022-09-12T23:59:35","DBAU 225057","Completed","2022-09-17T23:59:35","No","No","No","Internal","Office raised and items have been supplied in Singapore. Please confirm same has been received and renewed."]
[null,null,null,27471,63322,"24_Fri Sep 02 2022 23:18:08 GMT+0800","2022-08-22T23:59:35","Defect","Ship Staff","Engineering Audit","EGCS Sea water inlet line at the scrubber tower holed","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.31","Very High","","","welded the holed section","2022-10-31T23:59:35","","Completed","2022-09-03T23:59:35","No","No","No","Internal"]
[null,null,null,27448,35737,"24_Fri Sep 02 2022 23:54:27 GMT+0800","2022-08-23T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Few cargo and ballast valves operating switches have broken and brittle.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.11","Medium","","","Rec'd spares at Singapore. All 4 Switches renewed. Job completed.","2023-01-27T23:59:35","DBAU220175","Completed","2023-01-28T23:59:35","No","No","No","Internal","Order has been placed and estimated readiness is 30th November 2022. \nInspection is selected as Engineering Audit but Observer code is marked as SHIP STAFF. Please correct this."]
[null,null,null,27455,73007,"24_Sat Sep 17 2022 19:45:19 GMT+0800","2022-09-06T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Ejector pump casing is cracked due to erosion","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","New pump casing fixed in place - pump tried out satisfactorily.","2023-05-29T23:59:35","DBAU220188","Completed","2023-05-27T23:59:35","No","No","No","Internal","Long lead time for spare."]
[null,null,null,27512,42813,"24_Sat Sep 17 2022 19:42:20 GMT+0800","2022-09-06T23:59:35","Defect","Ship Staff","Ship Staff Insp.","UV Infra red fire tester defective","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.35","Medium","","","New tester tried out found working satisfactorily.","2022-12-05T23:59:35","DBAU220191","Completed","2022-10-29T23:59:35","No","No","No","Internal","Order has been placed and will be supplied in Singapore. \nIncorrect VIQ number has been mentioned. Please correct the same."]
[null,null,null,27454,11400,"24_Fri Sep 16 2022 18:40:37 GMT+0800","2022-09-07T23:59:35","Observation","Ship Staff","Ship Staff Insp.","No 2 Cargo Pump  AUS Pneumatic discharge valve  not remotely operated  from CCR.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.8","Medium","","","To be investigated After discharge Operation at Sriracha, and if spares required, spare  requisition to be raised.\nRepairs carried out.  Opening and closing fully during discharge operation at Singapore SRC terminal.","2022-10-07T23:59:35","","Completed","2022-10-17T23:59:35","No","No","No","Internal","Please revert with the trouble shooting results."]
[null,null,null,27479,30622,"24_Fri Sep 16 2022 22:41:32 GMT+0800","2022-09-07T23:59:35","Observation","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","The cross over platform gratings located at the cargo deck midships section noted with moderate rust condition","Deck - Pipe / Fittings","General Appearance","External Factors","11.3","Medium","","","corroded gratings replaced with new gratings received at Singapore 23 Sept 2022","2022-12-07T23:59:35","DBAU 220194","Completed","2022-09-17T23:59:35","No","No","No","External","Spares have been supplied in Singapore. Please renew all the gratings."]
[null,null,null,27447,10488,"24_Tue Oct 04 2022 01:00:59 GMT+0800","2022-09-21T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Ship Staff Insp.","Few grease point for gangway found to be dis connected from the grease nipple area.","Deck - Machinery","Safety / LSA / FFA","Equipment Related","5.47","Medium","","","Missing grease nipple to be connected and greasing to be carried out.\nAwaiting new grease nipples.  \nR.O number DBAU 220232\nGreasing carried out for gangway.  Disconnected grease line connected.","2022-10-01T23:59:35","","Completed","2022-11-07T23:59:35","No","No","No","Internal","Stores will be supplied in Singapore. Till then use grease nipples from other location and carry out greasing where the nipples are missing."]
[null,null,null,27460,70303,"24_Tue Oct 04 2022 00:57:03 GMT+0800","2022-09-21T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Vertical ladders leading to pump room blower motors found rusted.   Ladder to be de rusted and painted.","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.4","Very High","","","  Cosmetic upgrade completed.","2022-11-16T23:59:35","","Completed","2022-11-24T23:59:35","No","No","No","Internal"]
[null,null,null,27461,55326,"24_Tue Oct 04 2022 00:53:17 GMT+0800","2022-09-21T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","F-Spanner found missing from several fire hydrants on deck and Engine room.  Each fire hydrant to have dedicated F spanner.","","Safety / LSA / FFA","Inappropriate Procedure","12.15","High","","","F spanner  to be fabricated by fitter and placed near hydrants.","2022-10-01T23:59:35","","Completed","2022-09-25T23:59:35","No","No","No","Internal"]
[null,null,null,27497,23072,"24_Tue Oct 04 2022 00:53:31 GMT+0800","2022-09-21T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","M/E Fuel oil circulating pump no.2 found leaking","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Overhauled the pump and renewed the mechanical seals.","2022-10-15T23:59:35","","Completed","2022-09-17T23:59:35","No","No","No","Internal"]
[null,null,null,27501,90966,"24_Tue Oct 04 2022 00:57:48 GMT+0800","2022-09-21T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Ball valve found installed on main engine air starting line forward of the engine. No obstruction should be there for drain line as this is a safety measure. ","E/R - Main Engine","Eng. / Strg. Comp.","Inappropriate Procedure","10.32","Very High","","","Removed the valve and all advised not to put the valve in future.","2022-09-17T23:59:35","","Completed","2022-09-17T23:59:35","No","No","No","Internal"]
[null,null,null,27502,24793,"24_Tue Oct 04 2022 01:01:26 GMT+0800","2022-09-21T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Cylinder oil daily tank gauge glass found gagged with stoppers on both ends.","Miscellaneous","Eng. / Strg. Comp.","Inappropriate Procedure","10.25","Very High","","","Removed the gag tool and inspected all staff not to do the same in future.","2022-09-17T23:59:35","","Completed","2022-09-17T23:59:35","No","No","No","Internal"]
[null,null,null,27503,47592,"24_Tue Oct 04 2022 00:46:33 GMT+0800","2022-09-21T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Suction Strainer for Stbd fixed wilden pump on deck found corroded and damaged.  Vessel to replace strainer with new spares.","Deck - Machinery","MARPOL Related","Equipment Related","1.4","Low","","","Suction strainer cover made with SUS mesh and replaced on Port and Starboard side Wilden Pump","2022-11-16T23:59:35","","Completed","2022-09-29T23:59:35","No","No","No","Internal"]
[null,null,null,27504,26820,"24_Tue Oct 04 2022 00:59:53 GMT+0800","2022-09-21T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Several leaks observed on all 3 A/Es. Oil soaked rags were found under 2 AEs crankcase doors and under the fuel duplex filters.","E/R - Aux. Engine","Eng. / Strg. Comp.","Inappropriate Procedure","10.19","Very High","","","Rectified all leaks.","2022-10-01T23:59:35","","Completed","2022-09-26T23:59:35","No","No","No","Internal"]
[null,null,null,27505,26897,"24_Tue Oct 04 2022 00:55:28 GMT+0800","2022-09-21T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","M/E All units fuel pump tray area found with oil accumulation and oil soaked rags. Leaks to be identified. Oil soaked rags are not permitted anywhere in the engine room.","E/R - Main Engine","Eng. / Strg. Comp.","Inappropriate Procedure","10.19","Very High","","","Recitifed all leaks and cleaned the tray.","2022-10-01T23:59:35","","Completed","2022-09-29T23:59:35","No","No","No","Internal"]
[null,null,null,27507,89036,"24_Tue Oct 04 2022 01:04:06 GMT+0800","2022-09-21T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Hard board filing system on board not as per company procedure.  Please follow standard filing system fo all locations as per SMS.","Documentation","ISM Related","Inappropriate Procedure","","","","","Filing system redone  as per company SMS","2022-10-01T23:59:35","","Completed","2022-09-27T23:59:35","No","No","No","Internal"]
[null,null,null,27508,79702,"24_Tue Oct 04 2022 00:52:00 GMT+0800","2022-09-21T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Half cut tray found under boiler DO pilot pump in the purifier room. Tray was filled with oil. Leak needs to be identified and rectified. More leaks observed in the same area and DO was accumulated in the save all.","E/R - Pumps","Eng. / Strg. Comp.","Inappropriate Procedure","10.19","Very High","","","Tightened all couplings, rectified the leaks.","2022-09-27T23:59:35","","Completed","2022-09-26T23:59:35","No","No","No","Internal"]
[null,null,null,27520,98647,"24_Tue Oct 04 2022 01:07:14 GMT+0800","2022-09-21T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","All hydraulic line flanges in the fore castle to be covered with anti splash tape.","Deck - Machinery","Safety / LSA / FFA","Equipment Related","10.19","Very High","","","Anti Splash to be covered on all hydraulic flanges in fore peak store.\nJob completed.","2022-10-16T23:59:35","","Completed","2022-09-29T23:59:35","No","No","No","Internal"]
[null,null,null,28555,93436,"24_Wed Jan 18 2023 13:56:55 GMT+0800","2022-09-21T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Air found leaking from the Aft Main Engine Air Cooler when engine is running. Air leaking from aft cover at the bottom. ","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","O-Rings renewed and leak rectified.","2022-12-21T23:59:35","","Completed","2022-10-04T23:59:35","No","No","No","Internal"]
[null,null,null,27509,80132,"24_Mon Oct 03 2022 18:35:48 GMT+0800","2022-09-24T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Holed near No1 BWTS filter casing near bottom side.","","Structural Condn. / WT integrity ","Equipment Related","6.21","High","","","Temporary repair carried out.  Filter opened, candle filter removed and internal structure cleaned, and permanent repair carried out.  Internal structure to be painted with anti corrosive paint.","2022-10-13T23:59:35","","Completed","2022-10-13T23:59:35","No","No","No","Internal"]
[null,null,null,27506,15623,"24_Fri Oct 14 2022 00:51:31 GMT+0800","2022-09-26T23:59:35","Defect","Ship Staff","Ship Staff Insp.","No.1 M/E Auxiliary blower motor cooling fan found damaged","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Renewed the motor fan from spare and tried out found working satisfactory.","2022-12-07T23:59:35","","Completed","2022-09-28T23:59:35","No","No","No","Internal"]
[null,null,null,27510,50978,"24_Fri Oct 14 2022 00:55:31 GMT+0800","2022-09-27T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Temperature of veg and Diary room keeps fluctuating continuously and due to which solenoid valve keeps opening and closing continuously.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Renewed the control system from spare and tried out found working satisfactorily.","2022-10-24T23:59:35","","Completed","2022-10-05T23:59:35","No","No","No","Internal"]
[null,null,null,29556,60295,"0_Tue Mar 14 2023 14:38:31 GMT+0800","2022-10-05T23:59:35","Non Conformity","Ship Staff","Nav Audit / Verification","Vessel has 3 sets of GMDSS hand held walkie talkeis. Charger for one set not found working.","Navigation - GMDSS & Communication","Navigation","Equipment Related","4.23","High","","","Vessel has 3 sets of GMDSS walkie talkies and each of these have individual chargers. Presently vessel is using 2 chargers for all 3 walkie talkies. Complete one set of GMDSS radio with main battery, spare battery and charger has been ordered.","2023-01-05T23:59:35","","Completed","2022-10-28T23:59:35","No","No","No","Internal"]
[null,null,null,29557,73163,"0_Tue Mar 14 2023 14:41:11 GMT+0800","2022-10-05T23:59:35","Non Conformity","Ship Staff","Nav Audit / Verification","NAV-2 PC which acts as backup computer for ENC ordering and E Publications is freezing / gets hanged and very slow response.","Navigation - ECDIS","Navigation","Equipment Related","4.17","Very High","","","Vessel supplied with new NAV-2 laptop for replacing the outdated PC.","2023-01-05T23:59:35","","Completed","2022-10-06T23:59:35","No","No","No","Internal"]
[null,null,null,27464,55773,"24_Sun Oct 30 2022 19:56:06 GMT+0800","2022-10-09T23:59:35","Defect","Ship Staff","Ship Staff Insp.","M/E Fuel viscosity starter box found not working.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Viscosity starter box renewed, working satisfactory","2022-12-23T23:59:35","DBAU220213","Completed","2023-01-28T23:59:35","No","No","No","Internal","Send a separate mail wrt to all the trouble shooting you have carried out so that we can forward the same to makers for advise."]
[null,null,null,27449,82745,"24_Sun Oct 30 2022 19:57:57 GMT+0800","2022-10-10T23:59:35","Defect","Ship Staff","Ship Staff Insp.","No.2 Lub oil purifier temperature probe found defective.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Inspected and found the probe is not working.  already installed in place , lube oil purifier tried out and working satisfactory ","2023-08-10T23:59:35","DBAU220214","Completed",null,"No","No","No","Internal",""]
[null,null,null,27450,54619,"24_Sun Oct 30 2022 20:00:11 GMT+0800","2022-10-12T23:59:35","Defect","Ship Staff","Ship Staff Insp.","No.2 engine room blower starter in ESB found not working satisfactorily.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Spare MCCB of different type has been installed after making necessary modification.  Working satisfactory.  New spare received. Would be replaced at first available oppurtunity. ","2024-05-08T23:59:35","DBAU240081","Completed","2024-04-21T23:59:35","No","No","No","Internal","Spares have been ordered and will be supplied at Convenient port"]
[null,null,null,27451,76215,"24_Sun Oct 30 2022 20:02:11 GMT+0800","2022-10-15T23:59:35","Defect","Ship Staff","Ship Staff Insp.","EGCS Valve no.2070 actuating device found damaged.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","New actuator received, Same renewed.","2023-01-16T23:59:35","DBAU220223","Completed","2023-03-27T23:59:35","No","No","No","Internal","We are waiting for quotations from Makers. Intention is to supply at Singapore."]
[null,null,null,27511,23405,"24_Tue Oct 25 2022 16:25:16 GMT+0800","2022-10-18T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Stbd Life boat Canopy Light not working","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.28","Very High","","","Renewed the light from spare received at Singapore on 01/11/22.","2022-10-24T23:59:35"," DBAU220221","Completed","2022-10-27T23:59:35","No","No","No","Internal"]
[null,null,null,27453,72097,"24_Thu Nov 10 2022 12:37:14 GMT+0800","2022-10-24T23:59:35","Observation","Others (Eg. Insurance etc.)","Others (Eg. Insurance etc.)","Starboard LB release and retrieval system was found to be very tight for release and resetting.","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.28","Very High","","","Job deferred to drydock, specs raised in REFMAN.","2023-10-25T23:59:35","","Completed","2022-11-24T23:59:35","No","No","No","External","Enter this job scope in REFMAN and after that job to be closed from DDRL."]
[null,null,null,27457,94935,"24_Thu Nov 10 2022 12:42:21 GMT+0800","2022-10-24T23:59:35","Observation","Others (Eg. Insurance etc.)","Others (Eg. Insurance etc.)","Both LB’s breathing air regulator was found not functioning properly.","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.28","Very High","","","Air regulator renewed on Port ans Stbd side Lifeboats.","2023-01-24T23:59:35","DBAU220235","Completed","2023-01-30T23:59:35","No","No","No","External","PO approved. Will be supplied in Singapore"]
[null,null,null,27515,29614,"24_Thu Nov 10 2022 12:40:01 GMT+0800","2022-10-24T23:59:35","Observation","Others (Eg. Insurance etc.)","Others (Eg. Insurance etc.)","Both LB’s release hook shoe pins were found corroded. ","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.28","Very High","","","De-rusting and painting carried out","2023-01-24T23:59:35","","Completed","2022-10-27T23:59:35","No","No","No","External"]
[null,null,null,27516,38465,"24_Thu Nov 10 2022 12:45:05 GMT+0800","2022-10-24T23:59:35","Observation","Others (Eg. Insurance etc.)","Others (Eg. Insurance etc.)","Starboard davit – shackle for suspension block swivel piece was found corroded and thinned. ","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.28","Very High","","","After de-rusting noted that shackle is in satisfactory condition and does not require immediate replacement-However, will raise requisition for 2 shackles \n","2023-01-24T23:59:35"," DBAU220235 LIFEBOAT SPARES","Completed","2022-10-28T23:59:35","No","No","No","External"]
[null,null,null,27517,95043,"24_Thu Nov 10 2022 11:45:32 GMT+0800","2022-10-24T23:59:35","Observation","Others (Eg. Insurance etc.)","Others (Eg. Insurance etc.)","Starboard LB sprinkler suction valve was found seized.","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.28","Very High","","","Sprinkler valves have been overhauled and now are smooth in operation- Closed","2023-01-24T23:59:35","","Completed","2022-10-25T23:59:35","No","No","No","External"]
[null,null,null,27518,82156,"24_Thu Nov 10 2022 12:46:45 GMT+0800","2022-10-24T23:59:35","Observation","Others (Eg. Insurance etc.)","Others (Eg. Insurance etc.)","Port LB winch – Centrifugal brake units locking washer plate found missing.","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.28","Very High","","","Placed at location","2023-01-24T23:59:35","","Completed","2022-10-25T23:59:35","No","No","No","External"]
[null,null,null,27452,17725,"24_Thu Nov 10 2022 09:12:38 GMT+0800","2022-11-02T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Found few damaged candle filters, during Inspection and cleaning of No1 BWTS Filters.","Miscellaneous","Cargo / Ballast Systems","Equipment Related","6.21","High","","","BWTS No.1 filter unit opened and all filters cleaned. Found total 9 filters in damaged condition. All 9 filters were renewed. Job completed.","2023-03-27T23:59:35","DBAU 220238","Completed","2023-02-25T23:59:35","No","No","No","Internal","RO number is not mentioned in the relevant section. If the vessel has not yet raised RO then do not raise RO for new candles. Vessel to remove damaged candle filters from the filter stack. Please decrease the target date from one year to 6 months."]
[null,null,null,27730,52501,"24_Wed Nov 30 2022 23:32:01 GMT+0800","2022-11-11T23:59:35","Observation","Ship Staff","Ship Staff Insp.","The EGE door is found to be leaking off gas mildly on the stbd side.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Uneven surface of the mating surface welded and grounded by grinder for even surface finish, after taking approval from office. ","2022-12-25T23:59:35","","Completed","2022-11-17T23:59:35","No","No","No","Internal"]
[null,null,null,27729,38623,"24_Wed Nov 30 2022 23:40:09 GMT+0800","2022-11-13T23:59:35","Defect","Ship Staff","Ship Staff Insp.","No.2 Hydrophore pump pressure switch defective","E/R - Pumps,Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","pressure switch renewed","2023-02-12T23:59:35","DBAU220246","Completed","2023-01-16T23:59:35","No","No","No","Internal"]
[null,null,null,27728,88588,"24_Wed Nov 30 2022 23:47:00 GMT+0800","2022-11-14T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Workshop Air conditioner temperature switch found to faulty.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Temperature switch renewed, working satisfactory","2023-02-11T23:59:35","DBAU220247","Completed","2023-01-24T23:59:35","No","No","No","Internal"]
[null,null,null,27726,60006,"24_Wed Nov 30 2022 23:50:45 GMT+0800","2022-11-17T23:59:35","Defect","Ship Staff","Ship Staff Insp.","220V insulation found to be too low due to deck lights.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.38","Medium","","","Major low insulation found to be from Deck flood lights igniter,  many igniters replaced - work in progress. Many lights are already repaired and IS UNDER OBSERVATION. Present insulation improved and no alarm received in last few days. ","2023-08-30T23:59:35","","Completed","2023-08-11T23:59:35","No","No","No","Internal",""]
[null,null,null,27731,94804,"24_Wed Nov 30 2022 23:35:43 GMT+0800","2022-11-18T23:59:35","Observation","Ship Staff","Ship Staff Insp.","During scavenge inspection observed the No.2 fuel injector for unit no.6 was suspected to be leaking.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","To be renewed at convenient opportunity.","2022-12-05T23:59:35","","Completed","2022-11-19T23:59:35","No","No","No","Internal"]
[null,null,null,27725,23062,"24_Tue Nov 29 2022 21:08:12 GMT+0800","2022-11-24T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Port and stbd side gangway getting stuck in the dent on the track way. Metal plate thinned down and bent, also having hairline crack at 1 location on port gangway trackway.  ","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","Equipment Related","5.47","Medium","","","Temporary repairs carried out by pipes to raise and support the track way in place.  Additionally, defective sections of trackway rebuilt using weld filling and grinding done to even out the surface. Permanent repairs to be carried out in dry dock by renewal of complete H-channel.","2023-10-25T23:59:35","","Completed","2023-05-06T23:59:35","No","No","No","Internal"]
[null,null,null,27727,85198,"24_Tue Nov 29 2022 21:15:27 GMT+0800","2022-11-24T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","Deck Hydro blaster dump gun found leaking , and hydro blaster out of service.","Deck - Machinery","General Appearance","Equipment Related","11.10","Medium","","","Hydro blaster booster pump overhaul carried out with received spares at Singapore on 21-Nov-2023. Hydroblaster tried out & operational.","2023-10-31T23:59:35","","Completed","2023-11-26T23:59:35","No","No","No","Internal",""]
[null,null,null,27931,78930,"24_Thu Dec 15 2022 16:09:07 GMT+0800","2022-11-27T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Reefer heat exchanger found leaking","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Heat exchanger replaced with new one by yard and pressure tested after installation.","2023-10-31T23:59:35","DBAU220248 & DBAU220254","Completed","2024-02-23T23:59:35","No","No","No","Internal"]
[null,null,null,27934,18857,"24_Thu Dec 15 2022 16:10:47 GMT+0800","2022-12-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Fish room temperature controller found temperature variation was excess","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Renewed board from available old spare, working good.\nNew board received and stand by.","2023-03-01T23:59:35","DBAU220252","Completed","2023-03-24T23:59:35","No","No","No","Internal"]
[null,null,null,27932,52756,"24_Thu Dec 15 2022 16:05:38 GMT+0800","2022-12-03T23:59:35","Defect","Ship Staff","Ship Staff Insp.","No.2 IG Oxygen analyser sensor found not working","Inert Gas","Eng. / Strg. Comp.","Equipment Related","8.26","High","","","Sensor renewed, caliberation carried out, working satisfactory.","2023-03-03T23:59:35","DBAU220260","Completed","2023-01-21T23:59:35","No","No","No","Internal"]
[null,null,null,27933,50294,"24_Sun Dec 11 2022 09:23:25 GMT+0800","2022-12-07T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Poop deck Save all trays side plates found corroded and thinned down .","Deck - Pipe / Fittings","MARPOL Related","External Factors","6.9","Low","","","Temporary repairs carried out.  Side plates to be cropped and renewed with new plate at next dry docking period. Please advise if job to be transferred to REFMAN and close in DDRL.\nWork completed in drydock.","2024-02-29T23:59:35","","Completed","2024-03-06T23:59:35","No","No","No","Internal","Job to be transferred to REFMAN."]
[null,null,null,28102,63778,"24_Sun Jan 01 2023 18:19:10 GMT+0800","2022-12-27T23:59:35","Critical Equipment","Ship Staff","Ship Staff Insp.","Emergency Generator ACB found not operating satisfactorily.","Elect. Mach. & Equip.","Emgcy. Systems","Equipment Related","10.32","Very High","","","ACB  servicing carried out by shore technicians, UVT controller renewed.","2023-03-17T23:59:35","","Completed","2023-01-13T23:59:35","No","No","No","Internal"]
[null,null,null,28101,84867,"24_Sun Jan 01 2023 11:55:51 GMT+0800","2022-12-28T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Port lifeboat air supply system was found  leaking from No 1 and No 3 air bottle hoses. Leaks was observed both at manifold connection and at air bottle connection. Stbd side lifeboat were also found leaking from manifold.\n","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.29","High","","","No 3 bottle leak was rectified by welding the hose connector coupling at bottle end and using Teflon o-ring at manifold end. For no.1 bottle manifold connector there is still a leak and we are trying to arrest same. The leak at no.1 bottle connector was rectified by welding coupling connector.  These spares are under order DBAU220237 which are due for supply at Singapore. Rec'd spares, however main air supply valve and air bottle connecting hose connection donot match. Same has been informed to office. Temporary adaptor fabricated and fitted with new assembly and old main air supply valve on Port and stbd side lifeboat. New RO: DBAU230032 hasbeen raised for suitable adaptors for air manifold in order to connect Charging hose and air bottle hose together.\nAll connector replaced with newly received connectors.\n","2023-03-29T23:59:35","RO DBAU230032 ","Completed","2023-03-13T23:59:35","No","No","No","Internal"]
[null,null,null,28292,31018,"24_Sat Jan 14 2023 20:03:07 GMT+0800","2023-01-06T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Control air compressor hose to the heat exchanger is leaking, Hour meter is getting stuck sometimes.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","New hose fixed in place, compressor tried out observed no leaks. Hour meter working fine.","2023-04-28T23:59:35","DBAU230023","Completed","2023-04-16T23:59:35","No","No","No","Internal"]
[null,null,null,28294,39437,"24_Sat Jan 14 2023 16:24:01 GMT+0800","2023-01-07T23:59:35","Defect","Ship Staff","Ship Staff Insp.","ENGARD system reset button is not working","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","PCB was replaced by shore technician in drydock. working satisfactorily.","2023-10-30T23:59:35","DBAU230021","Completed","2024-02-23T23:59:35","No","No","No","Internal"]
[null,null,null,28295,73699,"24_Sat Jan 14 2023 13:31:04 GMT+0800","2023-01-09T23:59:35","Defect","Ship Staff","Ship Staff Insp.","BWTS  Feed pump no.2 leaking from mechanical seal.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Pump mechanical seal renewed. Pump tried out and found working satisfactory without any leaks.","2023-04-09T23:59:35","","Completed","2023-02-20T23:59:35","No","No","No","Internal"]
[null,null,null,28860,32191,"0_Sun Feb 26 2023 13:36:01 GMT+0800","2023-01-13T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Electrical wire management in the CCR was found very poor. This is a fire hazard. Please ensure this is rectified immediately","Miscellaneous","General Appearance","Human Error","11.16","Low","","","Cables neatly arranged and secured.","2023-04-12T23:59:35","","Completed","2023-03-20T23:59:35","No","No","No","Internal"]
[null,null,null,28862,77887,"0_Sun Feb 26 2023 14:31:13 GMT+0800","2023-01-13T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Pumproom rescue rope strands were found all opened up. ","Miscellaneous","ISM Related","Equipment Related","5.20","Medium","","","Pumproom rescue rope reseizing carried out.","2023-04-12T23:59:35","","Completed","2023-02-26T23:59:35","No","No","No","Internal"]
[null,null,null,28864,57602,"0_Sun Feb 26 2023 13:45:49 GMT+0800","2023-01-13T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Pump room davit - Hook lock found jammed. CA to be taken","Miscellaneous","ISM Related","Equipment Related","5.20","Medium","","","Pump room davit - Hook safety latch and spring fabricated and renewed.","2023-04-12T23:59:35","","Completed","2023-02-28T23:59:35","No","No","No","Internal"]
[null,null,null,28866,51569,"0_Sun Feb 26 2023 14:34:22 GMT+0800","2023-01-13T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Pump room bilge found very dirty condition - Needs proper upgrade. Include de-rusting and then do proper painting\n","Miscellaneous","Cargo / Ballast Systems","Human Error","8.44","High","","","Thorough cleaning carried out. Spot touch up carried out.","2023-05-23T23:59:35","","Completed","2023-05-23T23:59:35","No","No","No","Internal"]
[null,null,null,28867,44095,"0_Sun Feb 26 2023 14:17:50 GMT+0800","2023-01-13T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Starboard HHC - Luffing cylinder lower pin grease pipe found not in place.\n","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.50","Medium","","","New grease pipe fabricated and fitted. Jib completed.","2023-04-12T23:59:35","","Completed","2023-04-08T23:59:35","No","No","No","Internal"]
[null,null,null,28868,72395,"24_Sun Feb 26 2023 14:09:25 GMT+0800","2023-01-13T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Pump room blower motor external condition to be upgraded","Elect. Mach. & Equip.","General Appearance","Equipment Related","11.10","Medium","","","Pump room blower motor external condition upgradion completed, derusting and painting carried out.","2023-04-12T23:59:35","","Completed","2023-03-05T23:59:35","No","No","No","Internal"]
[null,null,null,28869,44982,"24_Tue Feb 28 2023 22:44:02 GMT+0800","2023-01-13T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Water ballast pump # 1 temperature sensor and wire needs to secured properly in place. ","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.8","Medium","","","Temperature sensor cable secured properly","2023-04-12T23:59:35","","Completed","2023-02-27T23:59:35","No","No","No","Internal"]
[null,null,null,28870,17978,"0_Sun Feb 26 2023 14:14:37 GMT+0800","2023-01-13T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Foam applicator springs on the deck found heavily rusted","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.40","Very High","","","Mechanical buffing of Foam applicator springs on deck carried out.","2023-06-12T23:59:35","","Completed","2023-05-31T23:59:35","No","No","No","Internal"]
[null,null,null,28871,92092,"0_Sun Feb 26 2023 13:37:23 GMT+0800","2023-01-13T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Bridge - File in the bridge was found broken.","Miscellaneous","General Appearance","Human Error","11.13","Low","","","Flie box/drawer to be repaired","2023-04-12T23:59:35","","Completed","2023-03-23T23:59:35","No","No","No","Internal"]
[null,null,null,28872,24184,"0_Sun Feb 26 2023 13:42:14 GMT+0800","2023-01-13T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","\tGratings on deck - Gratings at few places on deck found wasted and needs immediate attention. Spare material is there onboard and to be renewed.","Miscellaneous","General Appearance","Equipment Related","11.3","Medium","","","All damaged gratings renewal completed.","2023-04-12T23:59:35","","Completed","2023-02-28T23:59:35","No","No","No","Internal"]
[null,null,null,28873,98325,"0_Sun Feb 26 2023 13:44:02 GMT+0800","2023-01-13T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Natural exhaust vent for the Gymnasium - Securing butterfly nut found missing","Miscellaneous","General Appearance","Equipment Related","11.7","High","","","Butterfly bolt fabricated and fitted","2023-04-12T23:59:35","","Completed","2023-03-27T23:59:35","No","No","No","Internal"]
[null,null,null,28876,35036,"24_Sun Feb 26 2023 13:33:58 GMT+0800","2023-01-13T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","","Inert Gas,LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","REPAIRED","2023-04-12T23:59:35","","Completed","2023-02-22T23:59:35","No","No","No","Internal"]
[null,null,null,28877,67448,"0_Sun Feb 26 2023 14:29:00 GMT+0800","2023-01-13T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Fire bell support on deck found wasted.\n\n","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","Fire bell refitted at place ","2023-04-12T23:59:35","","Completed","2023-02-03T23:59:35","No","No","No","Internal"]
[null,null,null,28878,85092,"0_Sun Feb 26 2023 14:25:16 GMT+0800","2023-01-13T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Port HHC - Angle indicator for the HHC found missing\n\n","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.50","Medium","","","New angle indicator fabricated and fitted","2023-04-12T23:59:35","","Completed","2023-02-25T23:59:35","No","No","No","Internal"]
[null,null,null,28879,71744,"24_Sun Feb 26 2023 14:03:02 GMT+0800","2023-01-13T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Emergency light fittings - IWO pumproom on accommodation found secured with wire and heavily corroded.","Elect. Mach. & Equip.","General Appearance","Equipment Related","11.11","Very High","","","Complete light fitting renewed. Job completed.","2023-04-12T23:59:35","","Completed","2023-02-24T23:59:35","No","No","No","Internal"]
[null,null,null,28880,16379,"0_Sun Feb 26 2023 13:40:14 GMT+0800","2023-01-13T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Cable gland for the Port bridge wing light found holed. Please take CA","Miscellaneous","General Appearance","Human Error","11.10","Medium","","","Cable gland sealed. Job completed.","2023-04-12T23:59:35","","Completed","2023-02-24T23:59:35","No","No","No","Internal"]
[null,null,null,28881,39394,"0_Tue Feb 28 2023 22:48:15 GMT+0800","2023-01-13T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Flaps on Air ducts on the IG platform found jammed - same need to be eased up.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","5.35","Medium","","","Flaps eased up and now free to operate.","2023-04-12T23:59:35","","Completed","2023-02-07T23:59:35","No","No","No","Internal"]
[null,null,null,28882,77647,"0_Tue Feb 28 2023 22:51:03 GMT+0800","2023-01-13T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","EGCS - AE pressure transmitter pipeline flanges to be covered with lagging.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Flanges covered with lagging.","2023-04-12T23:59:35","","Completed","2023-02-24T23:59:35","No","No","No","Internal"]
[null,null,null,28883,10019,"24_Sun Feb 26 2023 14:22:16 GMT+0800","2023-01-13T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Securing wire for the bow stopper found broken","Deck - Mooring Machinery","Mooring","Equipment Related","9.20","Medium","","","New securing wire fixed to the bow stopper pin.","2023-04-12T23:59:35","","Completed","2023-02-03T23:59:35","No","No","No","Internal"]
[null,null,null,28884,82122,"0_Tue Feb 28 2023 22:53:20 GMT+0800","2023-01-13T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Excessive Gap on fixed Grinder in ER workshop. Gap to be adjusted.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","5.25","Medium","","","New grinding wheel fixed and gap adjusted.","2023-04-12T23:59:35","","Completed","2023-02-21T23:59:35","No","No","No","Internal"]
[null,null,null,30486,53528,"24_Fri Apr 21 2023 07:57:26 GMT+0800","2023-01-17T23:59:35","Defect","Ship Staff","Ship Staff Insp.","No.2 Ballast pump eductor found not working.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.8","Medium","","","On investigation it was observed that BWTS circulation valve BA515 found leaking. RO DBAU 230076 raised.\nValve BA 515  seat ring renewed and system tried out, found working satisfactory.","2023-04-16T23:59:35","RA230076","Completed","2023-04-17T23:59:35","No","No","No","Internal"]
[null,null,null,28552,57759,"24_Tue Jan 31 2023 12:15:01 GMT+0800","2023-01-17T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Main engine digital governor unit  inoperational","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Shore Technician visited at Fujairah on 02-Feb-2023 and renewed Regulator Process card. \nDGU waorking fine now.","2023-03-17T23:59:35","DBAU235013","Completed","2023-01-30T23:59:35","No","No","No","Internal"]
[null,null,null,28553,19063,"24_Wed Feb 01 2023 09:37:36 GMT+0800","2023-01-26T23:59:35","Observation","Ship Staff","Ship Staff Insp.","4 out of 6 personal gas detector H2S sensors are not working. Model GX-2009.","Miscellaneous","ISM Related","Equipment Related","5.23","Very High","","","All 4 personal gas meters serviced by Metromac at Fujairah on 10.Feb.2023. After servicing all 6 gas meters calibrated and found working satisfactory. Spare sensors also rec'd on 11.Feb.2023 at Fujairah vide RO: DBAU230027.","2023-04-25T23:59:35","DBAU230027","Completed","2023-02-07T23:59:35","No","No","No","Internal"]
[null,null,null,28554,60911,"24_Wed Feb 01 2023 09:41:52 GMT+0800","2023-01-26T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Few calibration gas ROB is nil (NItrogen & i-butane, H2S) for Portable gas meters i.e. RX-415 & RX-517, GX-8000, GX-8700. ","Miscellaneous","ISM Related","Equipment Related","5.23","Very High","","","Rec'd Calibration gases vide requisition DBAU230027 on 11.Feb 2023 at Fujairah. All portable and personnel gas meters calibrated and found working satisfactory.","2023-04-25T23:59:35","DBAU230027","Completed","2023-02-10T23:59:35","No","No","No","Internal"]
[null,null,null,28748,71709,"24_Wed Feb 15 2023 21:47:53 GMT+0800","2023-01-29T23:59:35","Other","Ship Staff","Ship Staff Insp.","EGCS SW Pipeline small section after valve 2170 was leaking, same repaired with welding and put back in use. Need to fabricate new section.  ","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Old section repaired and put back. New section fabricated and installed.","2023-05-02T23:59:35","","Completed","2023-04-26T23:59:35","No","No","No","Internal"]
[null,null,null,28750,43554,"24_Wed Feb 15 2023 22:57:46 GMT+0800","2023-01-29T23:59:35","Defect","Ship Staff","Ship Staff Insp.","440 Volt insulation found low.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.38","Medium","","","Observed galley Hot plates and oven giving low insulation. One hot plate renewed. Three hot plates and two oven heating element ordered.","2023-06-28T23:59:35","DBAU230035","Completed","2023-07-01T23:59:35","No","No","No","Internal","Spares supplied on 20th June. Please renew the damaged Hot Plate."]
[null,null,null,28859,10755,"0_Mon Feb 20 2023 15:09:45 GMT+0800","2023-01-30T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Few hydraulic hand pump for mooring winches brakes found not operational.","Deck - Mooring Machinery","Mooring","Equipment Related","9.14","Medium","","","Vessel overhauled 4 nos. of hydraulic brake pump and same replaced and tested. All pumps found leaking and unable to operate mooring winch brake. Additionally One more hand pump found not in working condition. Vessel has raised RO for new hand pumps. \nNew hand pump received and replaced. All mooring winches are working in good order.","2023-06-27T23:59:35","DBAU230071","Completed","2023-06-27T23:59:35","No","No","No","Internal"]
[null,null,null,28861,47255,"24_Mon Feb 20 2023 14:54:40 GMT+0800","2023-01-30T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Abnormal sound observed during operation of Port side hose handling crane. ","Deck - Machinery","Cargo / Ballast Systems","Equipment Related","8.50","Medium","","","As per GMTS technicians attended vsl at Fujairah on 02.feb.2023, abnormal sound coming due to worn out bushes of Jib hinge pin or lack of greasing. Greasing carried out of hinges by ship staff. However abnormal sound still coming. \n  GMTS technicians advised to change the worn out bushes. Worn out Bushes to be renewed at DD.\nTHOROUGH GREASING CARRIED OUT FOR THE CRANE. PORT SIDE HHC TRIED OUT SEVERAL TIMES AND FOUND NO SOUND COMING AS OF NOW. DEFECT BEING CLOSED. SHALL KEEP PORT HHC UNDER CLOSE OBSERVATION DURING OPERATION.","2023-08-30T23:59:35","","Completed","2023-08-07T23:59:35","No","No","No","Internal"]
[null,null,null,28863,46694,"0_Mon Feb 20 2023 15:00:10 GMT+0800","2023-01-30T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Few hydraulic connectors of Stbd hose handling crane were found rusted.  ","Deck - Machinery","Cargo / Ballast Systems","Human Error","8.50","Medium","","","All hydraulic fittings derusted and covered with denso tape.","2023-04-12T23:59:35","","Completed","2023-04-12T23:59:35","No","No","No","Internal"]
[null,null,null,28865,93963,"0_Mon Feb 20 2023 15:03:48 GMT+0800","2023-01-30T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Port and stbd provision crane limit switch bypass valve in-operational.","Deck - Machinery","ISM Related","Equipment Related","10.28","Low","","","New limit switch bypass valve installed. Working satisfactory. ","2024-06-06T23:59:35","","Completed","2024-04-20T23:59:35","No","No","No","Internal","All issues have been resolved in DD. Please close these items"]
[null,null,null,28874,56473,"0_Mon Feb 20 2023 15:06:39 GMT+0800","2023-01-30T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Stbd windlass fwd hydraulic motor flange on the gear box found to have minor leak during operation.","Deck - Mooring Machinery","Mooring","Equipment Related","9.20","Medium","","","GMTS technicians attended vsl at Fujairah on 11. Feb. 2023  and renewed the Lip seal of the hydraulic motor. Windlass tested and tried out after repairs and found working normal with no leaks.","2023-04-28T23:59:35","","Completed","2023-02-08T23:59:35","No","No","No","Internal"]
[null,null,null,28875,55926,"0_Mon Feb 20 2023 14:57:02 GMT+0800","2023-01-30T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Port side hose handling crane hoisting limit switch malfunctioning.","Deck - Machinery","Cargo / Ballast Systems","Equipment Related","8.50","Medium","","","Limit switch renewed by GMTS technicians on 11. Feb. 2023 and adjusted after renewal. Crane tested and tried out and found working normal. Limit switch supplied by vessel.","2023-04-28T23:59:35","","Completed","2023-02-08T23:59:35","No","No","No","Internal"]
[null,null,null,28751,52403,"24_Thu Feb 16 2023 03:22:01 GMT+0800","2023-01-31T23:59:35","Other","Ship Staff","Ship Staff Insp.","CRANE HYDRAULIC HOSES TO IDENTIFY AND UPDATE INVENTORY IN PAL.","Deck - Machinery","Eng. / Strg. Comp.","Equipment Related","","","","","CRANE HOSES IDENTIFIED, INVENTORY TAKEN AND REARRANGED.","2023-06-28T23:59:35","","Completed","2023-07-01T23:59:35","No","No","No","Internal","As this job is done this can be closed out in DDRL."]
[null,null,null,28749,91365,"24_Thu Feb 16 2023 03:28:13 GMT+0800","2023-02-07T23:59:35","Observation","Ship Staff","Ship Staff Insp.","SEWAGE COLLECTING TANK SOUNDING FLOAT MOVEMENT NOT SMOOTH. ","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","float pipe cleared. float movement checked. working satisfactory.","2023-05-07T23:59:35","","Completed","2023-04-17T23:59:35","No","No","No","Internal"]
[null,null,null,30497,12587,"24_Tue Jun 13 2023 11:46:33 GMT+0800","2023-03-12T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Engineering Audit","Energy Audit – Records of Last calibration of F.O. Flowmeters not available onboard.","Documentation","Cert. & Docu.","Equipment Related","","","","","Due to vessel schedule same could not be completed in stipulated time. same added to refman and will be carried out during drydock.\nDeferred to drydock.","2023-06-11T23:59:35","","Completed","2023-06-10T23:59:35","No","No","No","Internal"]
[null,null,null,29759,17583,"24_Sun Apr 16 2023 12:17:38 GMT+0800","2023-03-12T23:59:35","Defect","Ship Staff","Ship Staff Insp.","BWTS filter no.1  body holed and leaking","Deck - Machinery","Cargo / Ballast Systems","Equipment Related","8.18","High","","","Spare Filter Body received. Job to be carried out during DD. BWTS filter No.1 body has been repaired in DD in March 2024 using inserts . New body received was not used and kept in P/room .","2024-01-31T23:59:35","DBAU225042","Completed","2024-03-03T23:59:35","No","No","No","Internal"]
[null,null,null,29532,43472,"0_Thu Mar 23 2023 12:52:22 GMT+0800","2023-03-12T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","1P, 2P, 3P, FPK, APK Ballast tank Remote sounding gauge erratic","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.13","Medium","","","1P, 2P, 3P, FPK, ballast tanks inspected. All deck lines and lines inside tanks been blown through with compress air and water. All clogging cleared. Pressure transmitter/safety chamber tested and found in working condition. Tanks sounding to be tested during Ballast operation. APK tank remote gauging lines to be blown through and tested during tank inspection. All tanks level gauges calibrated after all lines cleared and pressure transmitter/safety chamber testing completed.\nGauges still not operational after servicing in drydock, have sent msg regarding the same to superintendent. Awaiting response.\n1.\tWe have checked free passage of the air line by water blowing, followed by air blowing the line, Caliberated the Zero and Span setting by pressure caliberator as per procedure in manual and size of the tank.\n2.\tObserved the Draft gauges to show accurate,\n3.\t3S,4 & 5 Ballast tanks reading are working satisfactory,\n4.\t2P Tank was working satisfactory but presently showing full reading due to blockage of line from deck to the tank, To clear the same at convenient opportunity,\n5.\t1P, 2S Air lines were blanked on top of the ballast tank and observed the reading to show full in the tank indicator, The lines are leaking inside the tank hence shows empty/Partial,\n6.\tFP, APT, 3P ballast tank Air line from the upper deck to Tank top is leaking, to identify the leak and rectify,\n7.\t1S Ballast tank is found to have mild leakage due to which the level does not show beyond 25M, To check for mild leak and rectify.\n8. Futher investigation to be carried out during load passage as ballast tanks will be empty.\n All lines, pressure transmitter checked for integrity and proper working. Dead sounding for the ballast tanks calibrated. Will check during ballasting operation at discharge port.\nGauges still not operational after servicing in drydock, have sent msg to superintendent and awaiting feedback. Vessel has renewed 4 faulty modulators in the electro-pneumatic panel and made system operational. System is under observation, current data is only having slight deviation, will raise this defect in case the deviation increases.","2024-05-29T23:59:35","","Completed","2024-05-25T23:59:35","No","No","No","Internal"]
[null,null,null,29533,45221,"0_Thu Mar 23 2023 14:11:33 GMT+0800","2023-03-12T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","AC Vent louvers on accommodation require derusting and cosmetic upgradation","Accommodation","General Appearance","Behaviour Based","11.1","High","","","AC Vent louvers on accommodation derusting and cosmetic upgradation carried out.","2023-04-12T23:59:35","","Completed","2023-03-31T23:59:35","No","No","No","Internal"]
[null,null,null,29534,37361,"0_Thu Mar 23 2023 14:13:18 GMT+0800","2023-03-12T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Nav Audit / Verification","4 nos lights foundation on Accommodation exterior thinned down and wasted.","Accommodation","General Appearance","Behaviour Based","11.10","Medium","","","Support brackets fabricated. ","2023-06-11T23:59:35","","Completed","2023-05-20T23:59:35","No","No","No","Internal"]
[null,null,null,29535,84076,"0_Thu Mar 23 2023 14:31:53 GMT+0800","2023-03-12T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Railings on Port side sunken deck bent on 2 locations","Deck - Pipe / Fittings","Safety / LSA / FFA","Behaviour Based","5.47","Medium","","","Railings on Port side sunken deck bent on 2 locations repaired.","2023-04-11T23:59:35","","Completed","2023-04-09T23:59:35","No","No","No","Internal"]
[null,null,null,29536,26439,"0_Thu Mar 23 2023 14:34:14 GMT+0800","2023-03-12T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Cargo Audit","Inert Gas (Main and Branch) lines on Deck having rust near flanges and U Clamps","Deck - Pipe / Fittings","Cargo / Ballast Systems","Behaviour Based","8.23","Medium","","","Inert Gas Main lines on Deck flanges and U Clamps derusting completed. Derusting of IG Branch lines, flanges and U Clamps in progress.\nVessel received new hydro blaster in Singapore and work will be undertaken along with deck cosmetic upgradation.\nVessel has been carrying out de-rusting on deck and pipelines  and conditional monitoring is in progress for the same. Maintenance issues on pipelines are being attended to on a priority basis.","2024-05-29T23:59:35","","Completed","2024-05-09T23:59:35","No","No","No","Internal"]
[null,null,null,29537,17463,"0_Thu Mar 23 2023 14:35:53 GMT+0800","2023-03-12T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Ship Staff Insp.","Foam monitors platform supports and grating require derusting and cosmetic upgradation.","LSA / FFA","Safety / LSA / FFA","Behaviour Based","5.40","Very High","","","Foam monitors platform supports and grating  derusting and cosmetic upgradation carried out..","2023-05-31T23:59:35","","Completed","2023-05-31T23:59:35","No","No","No","Internal"]
[null,null,null,29538,38336,"0_Thu Mar 23 2023 14:38:11 GMT+0800","2023-03-12T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Cargo Audit","Bosun Store Goose neck vent (P) rubber packing detoriated.","Hull & Tanks","General Appearance","Behaviour Based","11.7","High","","","Bosun Store Goose neck vent (P) rubber packing renewed.","2023-04-11T23:59:35","","Completed","2023-04-01T23:59:35","No","No","No","Internal"]
[null,null,null,29539,96704,"0_Thu Mar 23 2023 14:39:37 GMT+0800","2023-03-12T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Cargo Audit","TC034 COW Machine leaking","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.34","High","","","Spares received. Renewal of O-rings carried out. Leak repaired.","2023-09-29T23:59:35","DBAU230087 Received","Completed","2023-09-19T23:59:35","No","No","No","Internal","Spares will be supplied during next port call."]
[null,null,null,29540,40019,"0_Thu Mar 23 2023 14:19:35 GMT+0800","2023-03-12T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Cargo Audit","Butterworth manholes of 5P/C/S and Slop P/S require derusting and cosmetic upgradation.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Behaviour Based","11.6","Medium","","","Butterworth manholes of 5P/C/S and Slop P/S require derusting and cosmetic upgradation carried out.","2023-04-27T23:59:35","","Completed","2023-04-05T23:59:35","No","No","No","Internal"]
[null,null,null,29541,82959,"0_Thu Mar 23 2023 12:54:03 GMT+0800","2023-03-12T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Cargo Audit","Manifold pressure monitoring unit screen in CCR flickering","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.41","Medium","","","Manifold pressure monitoring unit screen renewed. \n","2023-05-12T23:59:35","DBAU235029","Completed","2023-05-11T23:59:35","No","No","No","Internal"]
[null,null,null,29542,66674,"24_Sun Mar 26 2023 17:46:54 GMT+0800","2023-03-12T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Boxes kept in spares locker of engine room not adequately lashed.","Miscellaneous","Eng. / Strg. Comp.","Behaviour Based","5.11","Low","","","Boxes re-arranged and lashed properly.","2023-05-17T23:59:35","","Completed","2023-05-27T23:59:35","No","No","No","Internal"]
[null,null,null,29543,51707,"24_Mon Mar 27 2023 00:08:12 GMT+0800","2023-03-12T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Purifier room door bent and not sealing fully on the bottom part.","Miscellaneous","Eng. / Strg. Comp.","Behaviour Based","5.34","Low","","","Door hinges adjusted, now sealing properly.","2023-04-27T23:59:35","","Completed","2023-04-07T23:59:35","No","No","No","Internal"]
[null,null,null,29544,19796,"24_Sun Mar 26 2023 18:03:18 GMT+0800","2023-03-12T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Meat room door rubber gasket worn out.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Meat room door rubber gasket renewed.","2023-06-27T23:59:35","DBAU230063","Completed","2023-07-13T23:59:35","No","No","No","Internal","Spares supplied under PO DBAU230063 in Singapore. Please renew this gasket and close out the defect."]
[null,null,null,29558,22828,"24_Sun Mar 26 2023 18:44:24 GMT+0800","2023-03-12T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Torn lagging near pipe below Vacuum condenser.","","Eng. / Strg. Comp.","Behaviour Based","10.19","Very High","","","Lagging renewed.","2023-03-22T23:59:35","","Completed","2023-03-20T23:59:35","No","No","No","Internal"]
[null,null,null,29559,66350,"24_Sun Mar 26 2023 18:48:20 GMT+0800","2023-03-12T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Oil leak near Aux Engine no 3 casing.","","Eng. / Strg. Comp.","Behaviour Based","10.29","Medium","","","Leak rectified.","2023-03-22T23:59:35","","Completed","2023-03-13T23:59:35","No","No","No","Internal"]
[null,null,null,29560,99917,"24_Sun Mar 26 2023 18:58:08 GMT+0800","2023-03-12T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Elevator escape hatch key glass casing broken.","Miscellaneous","Eng. / Strg. Comp.","Behaviour Based","","","","","Glass replaced.","2023-03-27T23:59:35","","Completed","2023-03-22T23:59:35","No","No","No","Internal"]
[null,null,null,29561,19611,"24_Thu Mar 23 2023 12:46:50 GMT+0800","2023-03-12T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","‘C’ Deck port side door closer broken","Accommodation","MLC Related","Behaviour Based","5.14","Very High","","","C’ Deck port side door closer repaired","2023-03-22T23:59:35","","Completed","2023-03-22T23:59:35","No","No","No","Internal"]
[null,null,null,29562,17954,"0_Thu Mar 23 2023 14:22:00 GMT+0800","2023-03-12T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Cargo Audit","2 nos foundation legs of Port Manifold drip tray corroded and wasted","Deck - Pipe / Fittings","Cargo / Ballast Systems","Behaviour Based","8.41","Medium","","","Fabrication and refitting of 2 nos foundation legs of Port Manifold drip tray completed.","2023-04-11T23:59:35","","Completed","2023-03-23T23:59:35","No","No","No","Internal"]
[null,null,null,29563,95825,"24_Sun Mar 26 2023 18:09:40 GMT+0800","2023-03-12T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Condensation water dripping from Vent in AC Room very close to Electrical panel.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.23","Medium","","","Panel covered with plastic sheet.","2023-03-21T23:59:35","","Completed","2023-03-13T23:59:35","No","No","No","Internal"]
[null,null,null,29564,26035,"24_Sun Mar 26 2023 18:24:34 GMT+0800","2023-03-12T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Loose lagging on ‘Steam to Slop tk heating valve’.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Behaviour Based","10.19","Very High","","","lagging on slop tank heating steam valve removed and put back properly.","2023-03-22T23:59:35","","Completed","2023-03-19T23:59:35","No","No","No","Internal"]
[null,null,null,29565,64219,"0_Thu Mar 23 2023 14:16:41 GMT+0800","2023-03-12T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","SOPEP Locker door rubber sealing lip thinned down and wasted.","Accommodation","General Appearance","Human Error","11.6","Medium","","","SOPEP Locker door rubber sealing lip fabrication completed.","2023-06-11T23:59:35","","Completed","2023-03-22T23:59:35","No","No","No","Internal"]
[null,null,null,29567,69554,"0_Thu Mar 23 2023 14:15:41 GMT+0800","2023-03-12T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","High Expansion foam door rubber sealing lip thinned down and wasted","Hull & Tanks","General Appearance","Behaviour Based","11.6","Medium","","","High Expansion foam door rubber sealing lip fabrication completed.","2023-06-11T23:59:35","","Completed","2023-03-22T23:59:35","No","No","No","Internal"]
[null,null,null,29568,79499,"0_Thu Mar 23 2023 14:28:33 GMT+0800","2023-03-12T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Cargo Audit","Pumproom Cofferdam Vent (S) mesh cover wasted","Deck - Pipe / Fittings","Cargo / Ballast Systems","Behaviour Based","8.53","Low","","","Pumproom Cofferdam Vent (S) mesh cover  fabricated and renewed.","2023-04-11T23:59:35","","Completed","2023-03-26T23:59:35","No","No","No","Internal"]
[null,null,null,29531,55406,"24_Mon Mar 20 2023 09:19:45 GMT+0800","2023-03-13T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Signal light coloum horn and rotating light not working on copt platform and near ECR","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.37","Medium","","","Horn and lights to renewed.","2023-06-12T23:59:35","DBAU230045","Completed","2023-05-21T23:59:35","No","No","No","Internal"]
[null,null,null,29762,86590,"24_Fri Apr 14 2023 22:46:10 GMT+0800","2023-04-09T23:59:35","Observation","Ship Staff","Ship Staff Insp.","During rounds observed abnormal noise from EGE sealing air fan.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","Fan stopped. Sealing air fan impeller and motor checked.  Found motor drive end bearing damaged, both bearings renewed ( driving and non driving end) renewed. Now working satisfactory.","2023-04-27T23:59:35","","Completed","2023-04-11T23:59:35","No","No","No","Internal"]
[null,null,null,29761,56181,"24_Sat Apr 15 2023 09:14:40 GMT+0800","2023-04-11T23:59:35","Observation","Ship Staff","Ship Staff Insp.","During routine rounds found sea water leakage from main sea water line. Main sea water line pressure transmitter connection came out from flange.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","wooden piece inserted to arrest sea water leakage. New flange fabricated for connection. Flange will be replaced at first opportunity.  Flange replaced during stoppage before singapore transit.","2023-05-28T23:59:35","","Completed","2023-04-13T23:59:35","No","No","No","Internal"]
[null,null,null,29758,82882,"24_Sun Apr 16 2023 07:45:06 GMT+0800","2023-04-12T23:59:35","Defect","Ship Staff","Ship Staff Insp.","EGE feed water pump # 2 motor controller malfunctioning","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.37","Medium","","","Motor controller  renewed.","2023-07-11T23:59:35","DBAU230069","Completed","2023-06-20T23:59:35","No","No","No","Internal"]
[null,null,null,30498,38537,"24_Tue Jun 06 2023 18:07:02 GMT+0800","2023-04-27T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Manifold marpol line valve found leaking during discharging operation at Lianyungang, china ","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.18","High","","","Seat ring renewed.","2023-05-17T23:59:35","","Completed","2023-05-13T23:59:35","No","No","No","Internal"]
[null,null,null,30487,41988,"24_Fri Jun 02 2023 01:41:26 GMT+0800","2023-05-08T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","EGCS room door open close marking missing.","Miscellaneous","Eng. / Strg. Comp.","Behaviour Based","","","","","Open close markings stenciled on the door.","2023-06-18T23:59:35","","Completed","2023-05-10T23:59:35","No","No","No","Internal"]
[null,null,null,30488,18424,"24_Fri Jun 02 2023 01:44:25 GMT+0800","2023-05-08T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Engine room funnel deck door securing bolt missing. To replace.","Miscellaneous","Eng. / Strg. Comp.","Human Error","","","","","Securing bolt put back in place","2023-06-18T23:59:35","","Completed","2023-05-10T23:59:35","No","No","No","Internal"]
[null,null,null,30489,86119,"24_Fri Jun 02 2023 01:47:05 GMT+0800","2023-05-08T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Drinking water cooler in accommodation filter renewal date  has crossed more than a year. To order and renew.","Miscellaneous","MLC Related","Equipment Related","","","","","Filters renewed.","2023-06-27T23:59:35","","Completed","2023-05-17T23:59:35","No","No","No","Internal"]
[null,null,null,30490,14478,"24_Fri Jun 02 2023 01:49:41 GMT+0800","2023-05-08T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ME no 6 fuel pump has sign of fuel oil leak. To identify and repair. ","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Leak from leak off line benzo bolt connection,same rectified.","2023-07-02T23:59:35","","Completed","2023-05-21T23:59:35","No","No","No","Internal"]
[null,null,null,30491,86286,"24_Tue Jun 06 2023 17:49:04 GMT+0800","2023-05-08T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Crew recreation room door handle damaged. To repair or renew.","Accommodation","MLC Related","Equipment Related","4.4","High","","","Crew recreation room door handle repaired.","2023-05-18T23:59:35","","Completed","2023-05-15T23:59:35","No","No","No","Internal"]
[null,null,null,30492,39845,"24_Fri Jun 02 2023 01:42:57 GMT+0800","2023-05-08T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Exhaust pipe between engine room and EGCS room in rusted condition.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","External Factors","","","","","Derusting and painting carried out","2023-06-23T23:59:35","","Completed","2023-05-12T23:59:35","No","No","No","Internal"]
[null,null,null,30493,84297,"0_Tue Jun 06 2023 17:55:52 GMT+0800","2023-05-08T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Life boat davit greasing points are not highlighted in yellow.","LSA / FFA","Safety / LSA / FFA","Behaviour Based","12.14","High","","","Life boat davit greasing points are highlighted in yellow.","2023-05-23T23:59:35","","Completed","2023-05-10T23:59:35","No","No","No","Internal"]
[null,null,null,30494,62627,"0_Tue Jun 06 2023 17:54:17 GMT+0800","2023-05-08T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Water collected in both water ballast pump save all. To clear and rectify the source of leak","Cargo Mach.","Cargo / Ballast Systems","Behaviour Based","8.44","High","","","Water collected in both water ballast pump save all cleared as it was due to the condensation.","2023-05-18T23:59:35","","Completed","2023-05-09T23:59:35","No","No","No","Internal"]
[null,null,null,35701,62344,"0_Sat Jun 01 2024 09:51:26 GMT+0800","2023-05-11T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Hydraulic boxes on main deck to derust and paint.","Deck - Pipe / Fittings","General Appearance","Equipment Related","","","","","All hydraulic boxes de-rusted and painted","2023-06-11T23:59:35","","Completed","2023-06-09T23:59:35","No","No","No","Internal","Regular inspection and maintenance to be carried out."]
[null,null,null,35702,39544,"24_Sat Jun 01 2024 09:49:10 GMT+0800","2023-05-11T23:59:35","Breakdown","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Area outside emergency DG room having lots of rust weep marks. To derust and paint.","Deck - Pipe / Fittings","General Appearance","Equipment Related","","","","","De-rusting completed and area painted.","2023-06-11T23:59:35","","Completed","2023-06-09T23:59:35","No","No","No","Internal"]
[null,null,null,30472,40638,"24_Fri Jun 02 2023 02:07:27 GMT+0800","2023-05-13T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Main engine fuel oil flowmeter not working.","","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Flowmeter transmitter faulty, reqisition DBAU230104 raised for same. Service Technician attended the vessel at Singapore on 21-Nov-2023. Flow meter made operational & in use.","2023-10-30T23:59:35","DBAU230104","Completed","2023-11-21T23:59:35","No","No","No","Internal"]
[null,null,null,30473,16432,"24_Fri Jun 02 2023 02:11:26 GMT+0800","2023-05-13T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Main Engine unit no 2 VIT rack stuck and Actuator linkage broken.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Fuel pump VIT actuator was overhauled in drydock by shore technician.","2023-10-30T23:59:35","DBAU230108","Completed","2024-03-16T23:59:35","No","No","No","Internal"]
[null,null,null,30474,34371,"24_Fri Jun 09 2023 16:56:01 GMT+0800","2023-05-21T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Main engine unit #7 crankpin bearing damage.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Crank pin bearing renewed by attending Shore team. In order.","2023-10-30T23:59:35","","Completed","2023-11-22T23:59:35","No","No","No","Internal"]
[null,null,null,30481,89280,"24_Fri Jun 02 2023 20:22:20 GMT+0800","2023-05-23T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Light signal column near incinarator not working, PCB defective.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.37","Medium","","","PCB needs to be renew. Requisition (DBAU230109) received in singapore and intalled in place , now Light signal Column working satisfactory ","2023-09-30T23:59:35","DBAU230109","Completed","2023-09-27T23:59:35","No","No","No","Internal","Spare will be supplied during next port call. Ready with forwarder"]
[null,null,null,30485,72203,"24_Fri Jun 09 2023 17:04:26 GMT+0800","2023-05-30T23:59:35","Defect","Ship Staff","Ship Staff Insp.","No 1 accomodation AC condensor gas leaked. found condensor cracked near motor foundation.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Welding repair carried out. Pressure carried out. Several leakages rectified. AC put in operation. ","2023-08-28T23:59:35","","Completed","2023-08-13T23:59:35","No","No","No","Internal"]
[null,null,null,30475,73262,"24_Fri Jun 09 2023 17:00:39 GMT+0800","2023-05-31T23:59:35","Defect","Ship Staff","Ship Staff Insp.","AE FO flowmeter (return) transmitter not working.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","AE FO flowmeter (return) transmitter to be renewed.  Service Technician attended the vessel at Singapore on 21-Nov-2023. Flow meter made operational & in use.","2023-10-31T23:59:35","DBAU230113","Completed","2023-11-21T23:59:35","No","No","No","Internal"]
[null,null,null,30482,66015,"24_Wed Jun 07 2023 01:22:05 GMT+0800","2023-05-31T23:59:35","Observation","Ship Staff","Ship Staff Insp.","PORT SIDE LIFE BOAT RUDDER IS NOT RESPONDING TO THE STEERING WHEEL","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.29","High","","","REPLACED THE WORNED OUT GEAR AND TRIED OUT, FOUND IN ORDER.","2023-08-30T23:59:35","","Completed","2023-07-04T23:59:35","No","No","No","Internal"]
[null,null,null,30496,38009,"24_Mon Jun 05 2023 15:04:10 GMT+0800","2023-05-31T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Port side lifeboat Diesel oil tank found leaking.","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.28","Very High","","","Leak to be arrested. Disel oil tank to be removed from locatrion and shifted to E/R workshop for pemanant repairs. Tank bottom plate renewed.","2023-08-30T23:59:35","","Completed","2023-06-08T23:59:35","No","No","No","Internal"]
[null,null,null,30477,83465,"24_Sat Jun 10 2023 10:22:39 GMT+0800","2023-06-02T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Fwd electric whistle not working. found piston and con rod damaged for horn.","Navigation - Others","Navigation","Equipment Related","10.32","Very High","","","Repairs carried out and tested, found in order.","2023-08-28T23:59:35","DBAU230116","Completed","2023-07-04T23:59:35","No","No","No","Internal"]
[null,null,null,30495,12556,"24_Wed Jun 07 2023 11:19:20 GMT+0800","2023-06-02T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Paint locker sprinkler system pipeline found corroded and wasted.","Deck - Pipe / Fittings,LSA / FFA","Safety / LSA / FFA","Equipment Related","5.35","Medium","","","Paint locker sprinkler system corroded and wasted pipeline fabricated, same replaced and tested.","2023-06-09T23:59:35","","Completed","2023-06-05T23:59:35","No","No","No","Internal"]
[null,null,null,30483,91402,"24_Sat Jun 17 2023 12:51:54 GMT+0800","2023-06-03T23:59:35","Observation","Ship Staff","Ship Staff Insp.","FW hydrophore No 1 pump rotating in reverse direction when pump is stop. Suction and discharge NRV not holding. ","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Pump changed over to no 2. No 1 pump valves renewed.","2023-08-03T23:59:35","DBAU230119","Completed","2023-07-23T23:59:35","No","No","No","Internal"]
[null,null,null,30476,73272,"24_Fri Jun 09 2023 17:27:59 GMT+0800","2023-06-05T23:59:35","Observation","Ship Staff","Ship Staff Insp.","BWTS electrolyser unit module securing plate found damaged due to overheat.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Regular cleaning and inspection is being carried out .  No further damage is observed.","2024-06-30T23:59:35","DBAU230137","Completed","2024-06-14T23:59:35","No","No","No","Internal","There is no further damage during regualr inspection and cleaning. Please close this defect as issue has been resolved."]
[null,null,null,30484,19629,"24_Mon Jun 12 2023 23:31:54 GMT+0800","2023-06-06T23:59:35","Observation","Ship Staff","Ship Staff Insp.","AIR LEAKING FROM EEBD CYLINDER PRESSURE REDUCER VALVE","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.44","High","","","EEBD CYLINDER PRESSURE REDUCER VALVE RENEWED AND TESTED, FOUND IN ORDER.","2023-09-05T23:59:35","","Completed","2023-07-04T23:59:35","No","No","No","Internal","Has the vessel issued PO for this item? No PO number is mentioned."]
[null,null,null,30479,72347,"24_Mon Jun 12 2023 18:55:44 GMT+0800","2023-06-09T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Main engine turbocharger no 1 inlet temp gauge not working.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","",". Vessel has fabricated one pocket and installed new temperature gauge .","2023-10-16T23:59:35","DBAU230119","Completed","2023-10-12T23:59:35","No","No","No","Internal","Spares have been supplied in Singapore. Please renew the temp gauge at the earliest."]
[null,null,null,30871,80605,"24_Sun Jul 02 2023 15:24:36 GMT+0800","2023-06-11T23:59:35","Observation","Ship Staff","Ship Staff Insp.","During pre arrival test for discharge port it was observed that the upper limit of port and Stbd HHC runner wire are misaligned.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.76","Medium","","","Port and Stbd HHC runner wire upper limit adjusted by adjusting camshaft on both the HHC.","2023-07-12T23:59:35","","Completed","2023-06-26T23:59:35","No","No","No","Internal"]
[null,null,null,30872,61379,"24_Sun Jul 02 2023 15:33:41 GMT+0800","2023-06-11T23:59:35","Observation","Ship Staff","Ship Staff Insp.","It was observed that slop port Inert gas inlet valve not holding","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.18","High","","","Defective valve renewed.","2023-06-27T23:59:35","","Completed","2023-06-27T23:59:35","No","No","No","Internal"]
[null,null,null,30862,18680,"24_Sun Jul 02 2023 15:38:48 GMT+0800","2023-06-17T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Railings for the side walk found rusted at several places. To be derusted","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.1","High","","","Railings for the side walk de-rusting Completed.","2023-09-16T23:59:35","","Completed","2023-07-12T23:59:35","No","No","No","Internal"]
[null,null,null,30863,79648,"24_Sun Jul 02 2023 15:40:47 GMT+0800","2023-06-17T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Steam smothering line on deck was renewed but painting of this pipe has not been carried out","Deck - Pipe / Fittings","General Appearance","Behaviour Based","11.1","High","","","Steam smothering line on deck was renewed and painted earlier but as the paint is heat resistance paint thus it peels off and requires regular maintenance which is Completed.","2023-08-16T23:59:35","","Completed","2023-07-13T23:59:35","No","No","No","Internal"]
[null,null,null,30864,65567,"24_Sun Jul 02 2023 15:42:24 GMT+0800","2023-06-17T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","PV Breaker Gauge glass securing foundation is heavily rusted.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Behaviour Based","8.28","Medium","","","PV Breaker gauge glass assembly fabricated and renewed.","2023-07-10T23:59:35","","Completed","2023-07-02T23:59:35","No","No","No","Internal"]
[null,null,null,30865,56758,"24_Sun Jul 02 2023 21:47:48 GMT+0800","2023-06-17T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Hydraulics - There are traces of oil leakage on top of aft hydraulic tank. ","Deck - Machinery","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Connections checked and tightened.","2023-07-12T23:59:35","","Completed","2023-07-19T23:59:35","No","No","No","Internal"]
[null,null,null,30866,71440,"24_Sun Jul 02 2023 21:49:40 GMT+0800","2023-06-17T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Few chain blocks found rusted.","Miscellaneous","Eng. / Strg. Comp.","Behaviour Based","10.28","Low","","","Chain Blocks cleaned/derusted and oiled. Load tested prior putting back in use.","2023-07-28T23:59:35","","Completed","2023-07-10T23:59:35","No","No","No","Internal"]
[null,null,null,30867,17174,"24_Sun Jul 02 2023 21:54:49 GMT+0800","2023-06-17T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Scupper drain pipe on the forward bulkhead of the VRCS unit is leaking. ","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","External Factors","10.31","Very High","","","Repaired.","2023-09-12T23:59:35","","Completed","2023-07-25T23:59:35","No","No","No","Internal"]
[null,null,null,30868,76708,"24_Sun Jul 02 2023 22:01:26 GMT+0800","2023-06-17T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ME LO filter - Middle section indication lever found missing","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","",""," New indication lever fitted.","2023-07-12T23:59:35","","Completed","2023-08-04T23:59:35","No","No","No","Internal"]
[null,null,null,30869,43568,"24_Sun Jul 02 2023 22:02:55 GMT+0800","2023-06-17T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","EGCS forward overboard valve - Manual wheel found missing.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Human Error,Behaviour Based","10.31","Very High","","","Wheel to put back in place.","2023-07-12T23:59:35","","Completed","2023-07-12T23:59:35","No","No","No","Internal"]
[null,null,null,30873,54428,"24_Sun Jul 02 2023 20:43:01 GMT+0800","2023-06-17T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ER Workshop - Grinder stone gap to be readjusted","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","Grinder stone gap to adjusted.","2023-07-12T23:59:35","","Completed","2023-06-29T23:59:35","No","No","No","Internal"]
[null,null,null,30874,19653,"24_Sun Jul 02 2023 21:56:40 GMT+0800","2023-06-17T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Ref compressor no 2 oil seal found leaking","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Seal renewed.","2023-07-12T23:59:35","","Completed","2023-06-19T23:59:35","No","No","No","Internal"]
[null,null,null,30875,29215,"24_Sun Jul 02 2023 21:58:41 GMT+0800","2023-06-17T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Air cooler upper drain pipe found disconnected.","E/R - Aux. Engine","Eng. / Strg. Comp.","Behaviour Based","10.31","Very High","","","Air cooler vent pipe connected.","2023-07-12T23:59:35","","Completed","2023-06-29T23:59:35","No","No","No","Internal"]
[null,null,null,30876,96200,"24_Sun Jul 02 2023 22:04:17 GMT+0800","2023-06-17T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Boiler blow down valve - DO NOT BLOW DOWN IN PORT poster missing.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Behaviour Based","10.31","Very High","","","poster put in place.","2023-07-12T23:59:35","","Completed","2023-06-29T23:59:35","No","No","No","Internal"]
[null,null,null,30877,25402,"24_Sun Jul 02 2023 22:52:55 GMT+0800","2023-06-21T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Emergency genrator battery exploded while starting emergency genrator.","Critical Equip.","Emgcy. Systems","Equipment Related","10.32","Very High","","","Starter checked for any defect. Battery isolated found shorted. Both batteries and isolator renewed. Emergency gen tried out, working satisfactory.","2023-07-28T23:59:35","","Completed","2023-06-24T23:59:35","No","No","No","Internal"]
[null,null,null,30870,84082,"24_Sun Jul 02 2023 22:57:27 GMT+0800","2023-06-23T23:59:35","Defect","Ship Staff","Ship Staff Insp.","AE 1 alternator reactor coil burnt.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","service engineer replaced L1 rector, AVR and one capacitor. Recomended to renew all capacitors and resistor.","2023-07-28T23:59:35","DBAU230110","Completed","2023-07-03T23:59:35","No","No","No","Internal"]
[null,null,null,30933,90068,"24_Mon Jul 17 2023 14:15:10 GMT+0800","2023-07-01T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Bunker tanks no.1 Port & no.1 Stbd holed from bulkhead near stairs support from Upper Deck to Sunken Poop deck.","Hull & Tanks","Structural Condn. / WT integrity ","External Factors","10.29","Medium","","","Temporary repairs carried out. As per office instructions, both bunker tanks to be filled to max 75% of the capacity. Permanent repairs have been completed in DD and vaccuum tests carried out satisfactorily . ","2024-01-31T23:59:35","","Completed","2024-03-09T23:59:35","Yes","No","No","Internal"]
[null,null,null,30931,41386,"24_Fri Jul 14 2023 10:08:59 GMT+0800","2023-07-09T23:59:35","Observation","Ship Staff","Ship Staff Insp.","5P COT IG PRESSURE SENSOR INOPERATIONAL","Inert Gas","Cargo / Ballast Systems","Equipment Related","8.19","High","","","IG PRESSURE TRANSMITTER RECEIVED & RENEWED FOR 5P COT. ","2023-10-09T23:59:35","DBAU230139","Completed","2023-08-13T23:59:35","No","No","No","Internal"]
[null,null,null,30932,33549,"24_Fri Jul 14 2023 10:16:31 GMT+0800","2023-07-10T23:59:35","Observation","Ship Staff","Ship Staff Insp.","STBD SIDE GANGWAY MOTOR FOUND WITH MINOR OIL LEAK","Deck - Machinery","ISM Related","Equipment Related","5.47","Medium","","","shifting winch taken to workshop, found too much oil filled. oil level reduced to requried level. bearings renewed. ","2023-10-10T23:59:35","","Completed","2023-07-19T23:59:35","No","No","No","Internal"]
[null,null,null,31151,54494,"24_Mon Aug 07 2023 21:02:25 GMT+0800","2023-07-29T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Sea water leakage from FWG ejector pump discharge valve body .","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.31","Very High","","","Req no DBAU230141 received in Singapore , discharge valve change with new one ,FWG ejector pump tested with new valve , FWG is in use.","2023-08-29T23:59:35","DBAU230141","Completed","2023-08-23T23:59:35","No","No","No","Internal"]
[null,null,null,31152,23501,"24_Mon Aug 07 2023 20:56:25 GMT+0800","2023-07-31T23:59:35","Defect","Ship Staff","Ship Staff Insp.","AE 1 Starting air motor not working.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Starting air motor renewed with new spare received. ","2023-10-30T23:59:35","DBAU235057","Completed","2023-08-08T23:59:35","No","No","No","Internal"]
[null,null,null,32022,67965,"24_Thu Aug 31 2023 09:30:49 GMT+0800","2023-08-09T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Ramp grating on deck i.w.o Slop Starboard side found rusted and needs attention.","Deck - Pipe / Fittings","General Appearance","External Factors","11.3","Medium","","","Ramp grating on deck iwo Slop Starboard side de-rusted & painted.","2023-11-30T23:59:35","","Completed","2023-11-08T23:59:35","No","No","No","Internal"]
[null,null,null,32023,54458,"24_Thu Aug 31 2023 09:41:41 GMT+0800","2023-08-09T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Starboard Gangway – Turn table bottom side has flake and rust formation. Need to be derusted.","Deck - Machinery","General Appearance","Equipment Related","5.47","Medium","","","Starboard Gangway – Turn table bottom side derusted and painted.","2023-10-24T23:59:35","","Completed","2023-10-14T23:59:35","No","No","No","Internal"]
[null,null,null,32024,44222,"24_Thu Aug 31 2023 09:46:21 GMT+0800","2023-08-09T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Foam monitor platform grating found rusted and needs derusting. Suggest to renew the grating with new.","Deck - Pipe / Fittings","General Appearance","External Factors","11.3","Medium","","","Foam monitor platform grating renewed.","2023-12-31T23:59:35","","Completed","2023-11-07T23:59:35","No","No","No","Internal"]
[null,null,null,32029,49799,"24_Thu Aug 31 2023 09:32:41 GMT+0800","2023-08-09T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Deck pipeline U bolts were found rusted and need immediate attention.","Deck - Pipe / Fittings","General Appearance","External Factors","11.5","Medium","","","Deck pipeline U bolts to be derusted and painted.","2023-12-31T23:59:35","","Completed","2023-11-04T23:59:35","No","No","No","Internal"]
[null,null,null,32030,23608,"24_Tue Aug 29 2023 18:37:32 GMT+0800","2023-08-09T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","MARSEC security level notice at the gangway still mentions vessel name as BW BAUHINIA.","Miscellaneous","Cert. & Docu.","Human Error","","","","","MARSEC security level notice at the gangway, vessel's name changed from BW BAUHINIA to DHT BAUHINIA.","2023-09-09T23:59:35","","Completed","2023-08-30T23:59:35","No","No","No","Internal"]
[null,null,null,32031,25027,"24_Thu Aug 31 2023 09:35:09 GMT+0800","2023-08-09T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Starboard gangway – metal support for the gangway mid-section of the gangway found rusted and needs immediate attention","Deck - Machinery","General Appearance","Equipment Related","5.47","Medium","","","Starboard gangway – metal support for the gangway mid-section of the gangway derusted and painted.","2023-09-09T23:59:35","","Completed","2023-08-30T23:59:35","No","No","No","Internal"]
[null,null,null,32032,52382,"24_Thu Aug 31 2023 16:44:52 GMT+0800","2023-08-09T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Bilge Holding tank sounding pipe threaded area was found damaged due to which sounding cap was not fully closed ","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","External Factors","10.26","High","","","Bilge holding tank sounding pipe threaded area refabricated and installed in place , ","2023-08-15T23:59:35","","Completed","2023-08-10T23:59:35","No","No","No","Internal","Bilge Holding tank sounding pipe threaded area was found damaged. To be renewed"]
[null,null,null,32033,61987,"24_Tue Aug 29 2023 18:31:49 GMT+0800","2023-08-09T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Fire door in the Officers Messroom found not closing properly. ","Accommodation","Safety / LSA / FFA","Equipment Related","5.35","Medium","","","Fire door in the Officers Messroom adjusted to close properly. ","2023-09-09T23:59:35","","Completed","2023-08-31T23:59:35","No","No","No","Internal"]
[null,null,null,29760,84188,"24_Sun Apr 16 2023 12:18:39 GMT+0800","2023-08-13T23:59:35","Defect","Ship Staff","Ship Staff Insp.","BWTS filter no.2 body holed at 2 places and leaking","Deck - Machinery","Cargo / Ballast Systems","Equipment Related","8.18","High","","","Soft repairs carried out. To be transferred in REFMAN for DD repairs. Permanent repairs have been completed in DD in March 2024 . Same Vaccuum tested and pressure tested satisfactory ","2024-01-31T23:59:35","","Completed","2024-03-03T23:59:35","No","No","No","Internal"]
[null,null,null,32026,46493,"24_Mon Sep 25 2023 20:59:55 GMT+0800","2023-08-30T23:59:35","Critical Equipment","Ship Staff","Ship Staff Insp.","Fixed Gas Detection System for Pump room Flow switch found getting stuck in between operation and triggering alarm, need to be renewed.\nO2 sensor reading not accurate, Sensor range 0-25% and reading showing 27%.","Critical Equip.","Safety / LSA / FFA","Equipment Related","5.17","Very High","","","Spares for renewal received and renewed.","2023-11-30T23:59:35","DBAU230158","Completed","2023-11-25T23:59:35","No","No","No","Internal"]
[null,null,null,32025,46270,"24_Sat Sep 09 2023 10:51:47 GMT+0800","2023-09-04T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Port Anchor Chain Studs detached welded part.","Deck - Mooring Machinery","Mooring","Equipment Related","9.20","Medium","","","Port Anchor Chain Studs to be rewelded during Dry Dock.\nJob completed in drydock","2024-01-31T23:59:35","","Completed","2024-03-17T23:59:35","No","No","No","Internal"]
[null,null,null,32035,68366,"24_Fri Sep 15 2023 09:47:33 GMT+0800","2023-09-04T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Bilge fire and GS Pump #2 Discharge valve gland not in good condition , sea water stains and salt were deposited ","Miscellaneous","Eng. / Strg. Comp.","External Factors","5.38","High","","","stains and salt deposits removed and Gland of discharge valve renewed with new one .","2023-09-06T23:59:35","","Completed","2023-09-05T23:59:35","No","No","No","Internal"]
[null,null,null,32038,92077,"24_Fri Sep 15 2023 10:48:24 GMT+0800","2023-09-04T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Main engine  leak off collecting funnel have fuel stains and lagging around pipes were in dirty condition ","E/R - Main Engine","Eng. / Strg. Comp.","Behaviour Based","10.19","Very High","","","Main engine leak off collecting unit cleaned and painted , all the lagging removed and renewed with new one ","2023-09-12T23:59:35","","Completed","2023-09-07T23:59:35","No","No","No","Internal"]
[null,null,null,32034,55600,"24_Fri Sep 15 2023 09:43:41 GMT+0800","2023-09-07T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Steam leakage from the warming up valve flange gasket and bonnet of warming up valve on COPT platform ","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Steam leak from the flange stopped by renewing the gasket. \nWarming up valve gland renewed with new one ","2023-09-09T23:59:35","","Completed","2023-09-08T23:59:35","No","No","No","Internal"]
[null,null,null,32037,39991,"24_Fri Sep 15 2023 10:45:16 GMT+0800","2023-09-07T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Slight leakage observed from the operating lever of mooring winch aft . The lever is also hard to move.","Deck - Mooring Machinery","Mooring","External Factors","9.15","Medium","","","Operating lever block overhauled. Seals renewed. Test run carried out satisfactorily. working smooth and no leakage present now.","2023-09-13T23:59:35","","Completed","2023-09-11T23:59:35","No","No","No","Internal"]
[null,null,null,32036,23975,"24_Fri Sep 15 2023 10:39:33 GMT+0800","2023-09-08T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Galley Ac providing insufficient cooling and indicator light for running was defective ","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","galley Ac charged with refer gas and indicator light renewed with new one","2023-09-12T23:59:35","","Completed","2023-09-10T23:59:35","No","No","No","Internal"]
[null,null,null,32028,23420,"24_Sat Sep 30 2023 19:37:08 GMT+0800","2023-09-22T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Ship Staff Insp.","Aux engine 2 and 3 over speed mechanical device to renew. ","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Aux engine 2 and 3 mechanical over-speed device overhauled and condition checked and found in order. New spares received, Shall be renewed as required. ","2024-03-08T23:59:35","","Completed","2024-03-20T23:59:35","No","No","No","Internal"]
[null,null,null,32027,39182,"24_Sat Sep 30 2023 19:30:33 GMT+0800","2023-09-26T23:59:35","Observation,Defect","Ship Staff","Ship Staff Insp.","Deck seal pump outlet line to deck seal leaking due to pin hole .","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.1","Medium","","","Leak arrested by cold repair. Permanent repair (hot work) carried out.","2023-12-26T23:59:35","NA","Completed","2023-12-01T23:59:35","No","No","No","Internal"]
[null,null,null,32039,64157,"24_Sun Oct 01 2023 11:33:18 GMT+0800","2023-09-28T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Aft winch Cooling water line from the lube cooler got pin hole .","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","External Factors","10.1","Medium","","","Pipe line removed and broght to the workshop for hot work , permanent repair carried out , same has been tested and found in order ","2023-09-29T23:59:35","","Completed","2023-09-28T23:59:35","No","No","No","Internal"]
[null,null,null,32355,57382,"24_Sun Oct 15 2023 14:27:08 GMT+0800","2023-10-04T23:59:35","Observation","Ship Staff","Ship Staff Insp.","common Control air dryer water drain unit leaking from the flexible pipe ","E/R - Air Comp.","Eng. / Strg. Comp.","External Factors","10.32","Very High","","","Auto drain system checked  ,flexible hose replaed with another one ","2023-10-15T23:59:35","","Completed","2023-10-09T23:59:35","No","No","No","Internal"]
[null,null,null,32354,51927,"24_Sun Oct 15 2023 14:17:24 GMT+0800","2023-10-05T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Service air compressor automatic drain line choked . ","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","service air compressor automatic drain system cleared , auto drain system cleaned , orfice checked . working satisafctory ","2023-10-15T23:59:35","","Completed","2023-10-06T23:59:35","No","No","No","Internal"]
[null,null,null,32358,60465,"24_Wed Nov 01 2023 10:08:57 GMT+0800","2023-10-09T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Mooring Winch Aft MW10 HP Line pipeline stub piece leaking.","Deck - Mooring Machinery","Mooring","Equipment Related","9.14","Medium","","","Hotwork carried out & stub section renewed. tried out & in order.","2024-01-09T23:59:35","NA","Completed","2023-10-09T23:59:35","No","No","No","Internal"]
[null,null,null,32359,61549,"0_Wed Nov 01 2023 10:12:15 GMT+0800","2023-10-14T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Vacuum System pump found cutting in frequently.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Flap valve found brittle & not sealing. Same renewed with onboard spare. RO raised for consummables.","2024-01-14T23:59:35","DBAU230181","Completed","2023-10-14T23:59:35","No","No","No","Internal"]
[null,null,null,32360,82420,"24_Wed Nov 01 2023 09:17:38 GMT+0800","2023-10-14T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Fire pump #1 Outlet Pipeline found leaking due to hole.","LSA / FFA,E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","5.38","High","",""," Pipe section renewed. Tried out & in use.","2024-01-14T23:59:35","NA","Completed","2023-10-20T23:59:35","No","No","No","Internal"]
[null,null,null,32341,66478,"0_Wed Nov 01 2023 09:19:20 GMT+0800","2023-10-16T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Fire Pump #1 Main Suction valve not holding. ","LSA / FFA,E/R - Pipes/ valves & fittings","Safety / LSA / FFA","Equipment Related","5.38","High","","","suction valve renewed with new spare valve in drydock by ship's staff.","2024-01-16T23:59:35","","Completed","2024-05-28T23:59:35","No","No","No","Internal"]
[null,null,null,32347,48628,"0_Wed Nov 01 2023 09:45:10 GMT+0800","2023-10-18T23:59:35","Observation","Ship Staff","Ship Staff Insp.","EGCS Absorber chamber shell damaged at two places bottom – crack on welding joint approx. 3 cm in length & Side of shell – damage on welding joint. ","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.11","Medium","","","Damaged portion was cut and renewed in drydock by yard, passification of same was carried out by ship's staff.","2024-01-18T23:59:35","NA","Completed","2024-03-17T23:59:35","No","No","No","Internal"]
[null,null,null,32348,88145,"0_Wed Nov 01 2023 09:49:20 GMT+0800","2023-10-18T23:59:35","Observation","Ship Staff","Ship Staff Insp.","EGCS SCS sample heater trouble. ","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.11","Medium","","","The heater was not able to maintain required temp. (55-60°C). Suspected internal loose connection in the heater. Gives “SCS Low temp alarm” intermittently.  Connection checked and issue rectified.  ","2024-04-18T23:59:35","NA","Completed","2024-04-17T23:59:35","No","No","No","Internal"]
[null,null,null,32357,82650,"0_Tue Oct 31 2023 14:20:51 GMT+0800","2023-10-19T23:59:35","Observation","Ship Staff","Ship Staff Insp.","AC Compressor #1 Shaft Seal found leaking & Crankcase oil discoloured. ","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Shaft seal renewed. Crankcase Oil renewed. RO raised for consumed spares.","2024-01-19T23:59:35","DBAU230197","Completed",null,"No","No","No","Internal"]
[null,null,null,32342,90448,"0_Wed Nov 01 2023 09:21:44 GMT+0800","2023-10-20T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Fire Pump #2 Outlet Valve is not holding. Pump rotating in opposite direction when #1 is running. ","LSA / FFA,E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","5.38","High","","","Valve renewed during dry-dock. Several operations has been carried out for observation. Valve confirmed holding good.  ","2024-05-08T23:59:35","","Completed","2024-05-08T23:59:35","No","No","No","Internal"]
[null,null,null,32353,83156,"0_Wed Nov 01 2023 10:03:23 GMT+0800","2023-10-20T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Incinerator operator panel “Comm Error Display-PLC”. ","Critical Equip.","MARPOL Related","Equipment Related","10.32","Very High","","","Maker advised renewal of the cable.  New cable received in singapore, same renewed and tried out.","2024-01-20T23:59:35","DBAU235070","Completed","2023-11-24T23:59:35","No","No","No","Internal"]
[null,null,null,32310,28343,"24_Tue Oct 31 2023 14:04:48 GMT+0800","2023-10-23T23:59:35","Observation","Ship Staff","Ship Staff Insp.","FWG Condenser Body found leaking due to crack.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Repaired in drydock by yard and pressure tested, found satisfactory.","2024-01-23T23:59:35","NA","Completed","2024-03-08T23:59:35","No","No","No","Internal"]
[null,null,null,32311,54970,"0_Tue Oct 31 2023 14:12:37 GMT+0800","2023-10-23T23:59:35","Observation","Ship Staff","Ship Staff Insp.","LT Cooler #2 Valves not holding.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Backflushing inlet valve was leaking, same renewed and checked by isolating cooler and opening vent, all valves are holding now.","2024-01-23T23:59:35","NA","Completed","2024-01-09T23:59:35","No","No","No","Internal"]
[null,null,null,32312,60612,"24_Tue Oct 31 2023 14:14:09 GMT+0800","2023-10-23T23:59:35","Observation","Ship Staff","Ship Staff Insp.","ME FO Circulating Pump #1 Mechanical Seal Leaking. ","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Same overhauled & boxed with new seal. Still Leaking slightly. Same re-opened. Found damage on the seal seating area on the pump body. Complete pump renewed with onboard new spare. Tried out & on stby.","2024-01-23T23:59:35","NA","Completed","2023-11-06T23:59:35","No","No","No","Internal"]
[null,null,null,32313,10031,"0_Tue Oct 31 2023 14:17:22 GMT+0800","2023-10-23T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Accommodation AC Compressor #1 coupling is damaged. ","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","New condenser unit installed and alignment carried out between compressor and motor by yard staff. Coupling renewed. Machinery is now operational.","2024-01-23T23:59:35","DBAU230197","Completed","2024-03-17T23:59:35","No","No","No","Internal"]
[null,null,null,32314,51688,"0_Tue Oct 31 2023 14:18:53 GMT+0800","2023-10-23T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Increased Vibration experienced when running both Accommodation Air Compressors are running. ","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Both Acc AC comp & motor laser alignment carried out in dry dock. Additional bracings fabricated and fit. Vibration has decreased considerable. Acc AC plant has been under observation since dry-dock and no increase in vibration noticed. Under observation. ","2024-05-08T23:59:35","","Completed","2024-05-08T23:59:35","No","No","No","Internal"]
[null,null,null,32315,22334,"0_Tue Oct 31 2023 14:24:10 GMT+0800","2023-10-23T23:59:35","Observation","Ship Staff","Ship Staff Insp.","440 V Insulation Low Intermittently.","Elect. Mach. & Equip.","General Appearance","Equipment Related","10.38","Medium","","","Galley equipment hot plates all cables renewed.  Under observation.","2024-05-23T23:59:35","","Completed","2024-05-15T23:59:35","No","No","No","Internal"]
[null,null,null,32316,76762,"24_Tue Oct 31 2023 14:27:01 GMT+0800","2023-10-23T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Galley Supply fan not operational.","Elect. Mach. & Equip.","General Appearance","Equipment Related","10.38","Medium","","","Low insulation from motor. Fan inspected. Found impeller stuck with casing due to rust/dirt. Same cleaned & painted. Boxed back & in use. Terminal block cover found heavily rusted. same renewed with onboard spare.","2024-01-23T23:59:35","NA","Completed","2023-11-11T23:59:35","No","No","No","Internal"]
[null,null,null,32317,57886,"0_Tue Oct 31 2023 14:29:03 GMT+0800","2023-10-23T23:59:35","Observation","Ship Staff","Ship Staff Insp.","220 V low insulation. ","Elect. Mach. & Equip.","General Appearance","Equipment Related","10.38","Medium","","","New fixture installed. Damaged wires renewed. 220V insulation >5 Mohm. ","2024-06-08T23:59:35","","Completed","2024-04-20T23:59:35","No","No","No","Internal"]
[null,null,null,32318,46969,"24_Tue Oct 31 2023 14:33:54 GMT+0800","2023-10-23T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Deck hydraulic lines needs renewal as condition is poor.","Deck - Machinery,Deck - Mooring Machinery,Deck - Pipe / Fittings","General Appearance","Equipment Related","11.4","Very High","","","Few already renewed and others in progress. RO raised for required piping/fittings.\nHydraulic Pipes changed which were leaking and rusty. Conitnous conditional monitoring is in progress and same is being attended to on priority basis.","2024-05-29T23:59:35","DBAU230195","Completed","2024-03-16T23:59:35","No","No","No","Internal","Specify which all section s tobe renewed."]
[null,null,null,32319,13939,"24_Tue Oct 31 2023 14:35:38 GMT+0800","2023-10-23T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Deck FW & Air Lines frequently have leaks. ","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.4","Very High","","","Few already renewed & others in progress. RO raised for piping/fittings.\nLeaks attended to as and when they are detected and pipes renewed, as required.","2024-05-29T23:59:35","DBAU230195","Completed","2024-05-21T23:59:35","No","No","No","Internal"]
[null,null,null,32320,57223,"0_Tue Oct 31 2023 14:38:30 GMT+0800","2023-10-23T23:59:35","Observation","Ship Staff","Ship Staff Insp.","EGB inlet bellow leaking. ","E/R - Boiler,E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","EGB inlet bellow replaced with new spare in drydock by yard.","2024-01-23T23:59:35","NA","Completed","2024-02-29T23:59:35","No","No","No","Internal"]
[null,null,null,32321,41999,"0_Tue Oct 31 2023 14:39:35 GMT+0800","2023-10-23T23:59:35","Observation","Ship Staff","Ship Staff Insp.","EGB casing holed near soot blower line penetration. ","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","casing repaired by riveting a doubler plate.","2024-01-23T23:59:35","","Completed","2023-11-17T23:59:35","No","No","No","Internal"]
[null,null,null,32322,86949,"0_Tue Oct 31 2023 14:43:59 GMT+0800","2023-10-23T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Stbd Windlass Hydraulic Motor(Fwd) Leak from the shaft seal.","Deck - Mooring Machinery","Mooring","Equipment Related","9.20","Medium","","","New motor on order. Awaiting supply.\nRegular monitoring in progress. No leakages observed during last operation.\nStbd windlass repaired and overauled in drydock and no leaks detected during operation post the completion of work.","2024-05-29T23:59:35","DBAU235066","Completed","2024-04-30T23:59:35","No","No","No","Internal"]
[null,null,null,32323,35675,"0_Tue Oct 31 2023 14:46:20 GMT+0800","2023-10-23T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Port Windlass Leak from the Operating block Pressure Relief valve. ","Deck - Mooring Machinery","Mooring","Equipment Related","9.20","Medium","","","The valve is heavily rusted & might break on opening. No spare onboard. RO raised.\nRegular monitoring in progress. No leakages observed during last operation in port.\nPort windlass overhauled in dry-dock and same has been observed having no leaks during operational usage.","2024-05-29T23:59:35","DBAU230196","Completed","2024-04-25T23:59:35","No","No","No","Internal"]
[null,null,null,32324,38403,"0_Tue Oct 31 2023 14:49:30 GMT+0800","2023-10-23T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Mooring Winch Hydraulic Brake Pumps frequently need repairing due to leaks/ unable to build pressure. ","Deck - Mooring Machinery","Mooring","Equipment Related","9.14","Medium","","","RO raised for spare pumps. Old units offlanded for renewal/overhaul at Singapore on 21-Nov-2023. Awaiting supply.\nNewly received pumps being changed and work in progress, will be completing the job this upcoming week.\nWork completed and new hand pumps renewed.","2024-06-14T23:59:35","DBAU230178 & DBAU230196","Completed","2024-04-18T23:59:35","No","No","No","Internal"]
[null,null,null,32325,43516,"0_Tue Oct 31 2023 14:56:24 GMT+0800","2023-10-23T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Drinking Water Fountain on B-Deck & ER not working. ","Accommodation","MLC Related","Equipment Related","11.16","Low","","","Both fountains renewed. ","2024-05-08T23:59:35","DBAU230165","Completed","2024-05-07T23:59:35","No","No","No","Internal"]
[null,null,null,32326,82289,"0_Tue Oct 31 2023 14:52:53 GMT+0800","2023-10-23T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Gas Cutting Oxygen Connecting hoses leaks at various locations. ","Miscellaneous","General Appearance","Equipment Related","5.26","Medium","","","Hoses renewed. ","2024-05-08T23:59:35","DBAU230169","Completed","2024-04-20T23:59:35","No","No","No","Internal"]
[null,null,null,32327,71326,"0_Tue Oct 31 2023 15:04:52 GMT+0800","2023-10-23T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Motor Switchboard Controllers for the following are defective. \nME Camshaft LO Booster Pump #2, Main FO Circulating pump #2 & Boiler Water Circulating Pump #2. \n","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.37","Medium","","","Camshaft & Boiler Water Circulating Pump #2 & ME Camshaft LO Booster Pump #2 controllers renewed with new received spares. Awaiting supply of pending controller for Main FO Ciculating Pump #2, under DBAU230231.","2024-01-23T23:59:35","DBAU230131","Completed","2023-11-24T23:59:35","No","No","No","Internal"]
[null,null,null,32328,12720,"0_Tue Oct 31 2023 15:07:44 GMT+0800","2023-10-23T23:59:35","Observation","Ship Staff","Ship Staff Insp.","FW UV sterilizer UV lamp not working. ","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.37","Medium","","","Spare received, renewed connecting cable and quartz sleeve, sterilizer tried out, working satisfactory.","2024-01-23T23:59:35","DBAU230136","Completed","2023-11-28T23:59:35","No","No","No","Internal"]
[null,null,null,32329,86734,"0_Tue Oct 31 2023 15:10:40 GMT+0800","2023-10-23T23:59:35","Observation","Ship Staff","Ship Staff Insp.","DO & HFO Bunker Lines have rust buildup.","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.4","Very High","","","Needs to be inspected after de-rusting. Pipeline to be renewed based on condition.\nCompleted in dry dock","2024-05-29T23:59:35","","Completed","2024-03-18T23:59:35","No","No","No","Internal","Pipelins have been renrewed in the DD. THis can be closed ."]
[null,null,null,32330,19692,"24_Tue Oct 31 2023 16:49:52 GMT+0800","2023-10-23T23:59:35","Observation","Ship Staff","Ship Staff Insp.","46.\tDeck water line (ER1 platform stbd side) needs renewal as pipeline holed at a few locations. ","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Deck service water line renewed in drydock by yard.","2024-01-23T23:59:35","NA","Completed","2024-03-08T23:59:35","No","No","No","Internal"]
[null,null,null,32331,26596,"0_Tue Oct 31 2023 16:51:51 GMT+0800","2023-10-23T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Deck seal pump suction line pinhole leak. ","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.31","Very High","","","Complete line & valve renewed with new spare. In order.","2024-01-23T23:59:35","NA","Completed","2023-11-07T23:59:35","No","No","No","Internal"]
[null,null,null,32332,26301,"0_Tue Oct 31 2023 16:58:59 GMT+0800","2023-10-23T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Galley meat room remote temperature gauge defective. ","Accommodation","General Appearance","Equipment Related","11.16","Low","","","Temp sensing bulb position changed. Defect rectified. ","2024-05-08T23:59:35","","Completed","2024-04-25T23:59:35","No","No","No","Internal",""]
[null,null,null,32333,40247,"0_Tue Oct 31 2023 14:59:01 GMT+0800","2023-10-23T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Aux boiler DO flowmeter not working. ","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Spare received at Singapore, same renewed. Flow meter working satisfactory.","2024-01-23T23:59:35","DBAU230170","Completed","2023-11-23T23:59:35","No","No","No","Internal"]
[null,null,null,32334,76060,"0_Tue Oct 31 2023 15:01:43 GMT+0800","2023-10-23T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Crew laundry washing machine & Officers laundry Dryer not operational. ","Accommodation","General Appearance","Equipment Related","11.16","Low","","","Crew laundry Washing repaired and made operational.","2024-01-23T23:59:35","DBAU230191","Completed","2024-03-07T23:59:35","No","No","No","Internal"]
[null,null,null,32335,73833,"0_Tue Oct 31 2023 17:02:14 GMT+0800","2023-10-23T23:59:35","Observation","Ship Staff","Ship Staff Insp.","440 V low insulation from ESB bus bar ","Elect. Mach. & Equip.","Emgcy. Systems","Equipment Related","10.38","Medium","","","Cleaning of ESB carried out at drydock and issue rectified.","2024-01-23T23:59:35","NA","Completed","2024-03-14T23:59:35","No","No","No","Internal"]
[null,null,null,32336,15428,"0_Tue Oct 31 2023 17:05:42 GMT+0800","2023-10-23T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Light signal column in Steering gear room not working.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.37","Medium","","","PCB fault. RO raised. Spares received at Singapore on 23-Dec-2023. Same installed & Light Signal column working.","2024-01-23T23:59:35","DBAU230187","Completed","2023-12-26T23:59:35","No","No","No","Internal"]
[null,null,null,32337,76261,"0_Tue Oct 31 2023 17:07:32 GMT+0800","2023-10-23T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Boiler control panel unit cooler is faulty. ","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Hermetic compressor giving low insulation. Unit cooler is operating on Fan mode only. Temp is being maintained.  Under observation.","2024-05-08T23:59:35","DBAU230135","Completed","2024-04-30T23:59:35","No","No","No","Internal",""]
[null,null,null,32338,55265,"0_Tue Oct 31 2023 17:09:18 GMT+0800","2023-10-23T23:59:35","Observation","Ship Staff","Ship Staff Insp.","ME maneuvering station sound powered telephone not working.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.37","Medium","","","Spare received at Singapore, same renewed and tried out, working satisfactory.","2024-01-23T23:59:35","DBAU230159","Completed","2023-11-25T23:59:35","No","No","No","Internal"]
[null,null,null,32339,33394,"0_Tue Oct 31 2023 17:14:39 GMT+0800","2023-10-23T23:59:35","Observation","Ship Staff","Ship Staff Insp.","COPT platform IS telephone faulty.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.37","Medium","","","Spare received at singapore, same renewed and tried out, working satisfactory.","2024-01-23T23:59:35","DBAU230159","Completed","2023-11-25T23:59:35","No","No","No","Internal"]
[null,null,null,32340,16116,"0_Tue Oct 31 2023 17:15:58 GMT+0800","2023-10-23T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Viscosity Controller not operational. ","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","As per maker the model is obsolete, need upgradation. Controller working on TEMP control. ","2024-05-08T23:59:35","","Completed","2024-04-18T23:59:35","No","No","No","Internal",""]
[null,null,null,32343,58132,"0_Wed Nov 01 2023 09:35:13 GMT+0800","2023-10-23T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Life boat winch handle support corroded.","LSA / FFA,Deck - Pipe / Fittings","Safety / LSA / FFA","Equipment Related","5.29","High","","","Handle supports renewed with fabricated spare.","2024-01-23T23:59:35","NA","Completed","2023-11-13T23:59:35","No","No","No","Internal"]
[null,null,null,32344,45190,"0_Wed Nov 01 2023 09:28:29 GMT+0800","2023-10-23T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Wilden pump base frame found corroded.","Critical Equip.,Deck - Machinery","MARPOL Related","Equipment Related","6.3","Low","","","New frame fabricated & installed.","2024-01-23T23:59:35","NA","Completed","2023-11-11T23:59:35","No","No","No","Internal"]
[null,null,null,32345,13204,"0_Wed Nov 01 2023 09:32:37 GMT+0800","2023-10-23T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Various Accommodation & ER doors handles faulty. ","Accommodation,Miscellaneous","General Appearance","Equipment Related","11.13","Low","","","Purifier room door closer adjusted. Accomodation doors be repaired. RO to be raised as required.\nWork completed in drydock.","2024-01-23T23:59:35","","Completed","2024-03-18T23:59:35","No","No","No","Internal"]
[null,null,null,32350,29517,"0_Wed Nov 01 2023 09:54:39 GMT+0800","2023-10-23T23:59:35","Observation","Ship Staff","Ship Staff Insp.","BWTS NU Pump #1 Differential Pressure transmitter faulty. ","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","6.21","High","","","RO raised. Spare received in Singapore and same renewed.","2024-01-23T23:59:35","DBAU230202","Completed","2023-11-27T23:59:35","No","No","No","Internal"]
[null,null,null,32351,38986,"0_Wed Nov 01 2023 09:59:19 GMT+0800","2023-10-23T23:59:35","Observation","Ship Staff","Ship Staff Insp.","IG O2 Analyser #2 showing an error of 0.6% even after calibration. ","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.26","High","","","Oxy analyzer sensor renewed. Callibration carried out. Found working satisfactory.","2024-05-08T23:59:35","","Completed","2024-04-16T23:59:35","No","No","No","Internal",""]
[null,null,null,32352,33897,"0_Wed Nov 01 2023 09:40:05 GMT+0800","2023-10-23T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Accommodation Gas detection system HC sensor faulty. ","Critical Equip.,Elect. Mach. & Equip.","Safety / LSA / FFA","Equipment Related","8.41","Medium","","","Sensor callibrated. Found working satisfactory.","2024-04-30T23:59:35","","Completed","2024-04-18T23:59:35","No","No","No","Internal",""]
[null,null,null,32356,89336,"0_Tue Oct 31 2023 14:16:18 GMT+0800","2023-10-23T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Accommodation AC Compressor #2 coupling was damaged. ","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Same was renewed from spares. Vessel is not having new spare flexible coupling. RO raised.","2024-01-23T23:59:35","DBAU230197","Completed","2023-10-23T23:59:35","No","No","No","Internal"]
[null,null,null,32818,51096,"24_Fri Nov 17 2023 10:16:49 GMT+0800","2023-10-29T23:59:35","Observation","Ship Staff","Ship Staff Insp.","MW7: Brake Cylinder leaking. Manual brake seized & unable to operate smoothly.","Deck - Mooring Machinery","Mooring","Equipment Related","9.14","Medium","","","Brake Cylinder renewed with onboard overhauled spare. \nBrake hydraulic hand pump renewed. ","2024-05-15T23:59:35","DBAU230196","Completed","2024-04-18T23:59:35","No","No","No","Internal",""]
[null,null,null,32824,35588,"24_Fri Nov 17 2023 08:35:28 GMT+0800","2023-10-29T23:59:35","Observation","Ship Staff","Ship Staff Insp.","AE#1 Fuel Pump Return Banjo Bolt leaking.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Banjo Bolt copper gasket renewed. ","2024-01-30T23:59:35","NA","Completed","2023-10-30T23:59:35","No","No","No","Internal"]
[null,null,null,32832,18585,"24_Fri Nov 17 2023 10:12:13 GMT+0800","2023-10-29T23:59:35","Observation","Ship Staff","Ship Staff Insp.","MW6 (Mid Port) Leak from the Main block Plug. \nMW8: Leak from the operating handle shaft seal.\nMW10: Leak from the Operating block Plug.","Deck - Mooring Machinery","Mooring","Equipment Related","9.14","Medium","","","MW6: Plug renewed with onboard new spare.\nMW8: Operating shaft block overhauled with new seals.\nMW10: plug renewed with onboard new spare.","2024-01-29T23:59:35","","Completed","2023-11-08T23:59:35","No","No","No","Internal"]
[null,null,null,32825,90326,"0_Fri Nov 17 2023 08:37:34 GMT+0800","2023-10-31T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Service Air Compressor Auto Drain Leaking","E/R - Aux. Mach.,E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Auto drain cleaned. Drain line also found holed. Same renewed.","2024-01-31T23:59:35","NA","Completed","2023-10-31T23:59:35","No","No","No","Internal"]
[null,null,null,32826,86573,"0_Fri Nov 17 2023 08:54:11 GMT+0800","2023-11-04T23:59:35","Observation","Ship Staff","Ship Staff Insp.","ME FO Circulating Pump #2 found leaking from the mechanical seal.","E/R - Pumps,E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Pump opened up & found the bearing damaged. Also noticed damage to the power rotor shaft where the bearing sits. Rotors renewed with new onboard spares. Pump tried out & in use. RO raised for required spares.","2024-02-04T23:59:35","","Completed","2023-11-04T23:59:35","No","No","No","Internal"]
[null,null,null,32831,23283,"0_Fri Nov 17 2023 09:02:08 GMT+0800","2023-11-05T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Atmospheric Condenser Cooling SW Pump Leaking during operation.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Pump opened up for inspection. Found the mech seal & shaft sleeve damaged. Same renewed. Mouth rings & line bearing clearances within limits. Pump boxed up, tried out & in use.","2024-02-07T23:59:35","","Completed","2023-11-07T23:59:35","No","No","No","Internal"]
[null,null,null,32811,37040,"0_Fri Nov 17 2023 08:57:01 GMT+0800","2023-11-06T23:59:35","Observation","Ship Staff","Ship Staff Insp.","ME Fuel Valve Testing Device Trouble.","E/R - Main Engine,Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","All parts of ME Fuel Valve Testing Device were cleaned. Device is working as of now and is under observation. ","2024-05-08T23:59:35","","Completed","2024-03-15T23:59:35","No","No","No","Internal","This issue was already resolved in DD."]
[null,null,null,32827,66832,"0_Fri Nov 17 2023 09:24:11 GMT+0800","2023-11-08T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Lifeboat (Port Side) Brake Lever Pin Bracket damaged.","Critical Equip.,Deck - Machinery","Eng. / Strg. Comp.","Equipment Related","5.29","High","","","New bracket fabricated & installed.","2024-02-08T23:59:35","NA","Completed","2023-11-13T23:59:35","No","No","No","Internal"]
[null,null,null,32830,47760,"24_Fri Nov 17 2023 10:08:49 GMT+0800","2023-11-09T23:59:35","Observation","Ship Staff","Ship Staff Insp.","AUS system control air leak in CCR, Leak observed from Gas extraction valve controlling solenoid valve.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.8","Medium","","","Solenoid valve renewed","2024-02-09T23:59:35","NA","Completed","2023-11-10T23:59:35","No","No","No","Internal"]
[null,null,null,32828,47274,"24_Fri Nov 17 2023 09:29:55 GMT+0800","2023-11-10T23:59:35","Observation","Ship Staff","Ship Staff Insp.","ME Pneumatic System Control Air Reduction Unit Valve 203 found leaking.","E/R - Main Engine,E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Valve overhauled using onboard overhaul kit. Tried out & in use.","2024-02-10T23:59:35","NA","Completed","2023-11-10T23:59:35","No","No","No","Internal"]
[null,null,null,32812,64812,"0_Fri Nov 17 2023 09:35:02 GMT+0800","2023-11-13T23:59:35","Critical Equipment","Ship Staff","Ship Staff Insp.","CO2 Bottle Bursting Disc to renew from Copper to Nickel.","Critical Equip.","Safety / LSA / FFA","Industry Issue","5.35","Medium","","","Health check already carrie dout and liquid measuring of the bottles carried out in DD. Management has decide not carry out bursting disc renewal basis other tests conducted.","2024-05-31T23:59:35","NA","Completed","2024-03-31T23:59:35","No","No","No","Internal","Health check already carrie dout and liquid measuring of the bottles carried out in DD. Management has decide not carry out bursting disc renewal basis other tests conducted. Job to be closed out."]
[null,null,null,32834,35824,"24_Fri Dec 01 2023 13:36:00 GMT+0800","2023-11-20T23:59:35","Observation","Ship Staff","Ship Staff Insp.","FW in accomodation found intermittently discoloured.","Accommodation,E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Shipstaff cleaned the FW Hydrophore Tank in Oct-2023. Found with small quantity of red deposit. same cleared. Shipstaff opened up the Re-Hardening Filter for inspection. Found with excessive red/black deposit. The filter was cleaned & dolomite elements renewed with new spare. FW Sterilizer filter also found dirty. Same renewed. System in use & no FW discoloration.","2024-02-27T23:59:35","","Completed","2023-11-28T23:59:35","No","No","No","Internal"]
[null,null,null,32813,92000,"24_Mon Nov 27 2023 05:12:50 GMT+0800","2023-11-21T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Supports/ cradles for stanchions (Pilot Ladder) eroded and wasted","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","Equipment Related","5.47","Medium","","","Supports/ cradles for stanchions (Pilot Ladder) eroded and wasted to be de-rusted and painted.\nCompleted.","2024-05-21T23:59:35","","Completed","2024-03-15T23:59:35","No","No","No","Internal"]
[null,null,null,32814,89682,"24_Mon Nov 27 2023 05:16:54 GMT+0800","2023-11-21T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Emergency operation connections of the crane to be highlighted. Manual pump to be identified/ procured and procedure to be made and posted.","Deck - Machinery","ISM Related","Inappropriate Procedure","8.50","Medium","","","New pump has been supplied to the vessel","2024-07-21T23:59:35","","Completed","2024-03-23T23:59:35","No","No","No","Internal","Emergency pump was supplied when vessel called Singapore in April after DD."]
[null,null,null,32815,93101,"24_Mon Nov 27 2023 05:20:39 GMT+0800","2023-11-21T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Manifold reducer flanges to be compared against ANSI standards for thickness and repaired as deemed necessary.","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","Equipment Related","8.41","Medium","","","Manifold reducer flanges to be compared against ANSI standards for thickness and repaired as deemed necessary.\nManifold reducer flanges are complying with ANSI standards.","2024-05-21T23:59:35","","Completed","2024-05-13T23:59:35","No","No","No","Internal"]
[null,null,null,32816,33955,"24_Mon Nov 27 2023 05:21:42 GMT+0800","2023-11-21T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Isolation valves (Fire and Foam) drain valves to be opened, and drained. Seats to be clean prior boxing back. Integrity of the valves to be tested.","Deck - Pipe / Fittings","Safety / LSA / FFA","Equipment Related","5.35","Medium","","","Isolation valves (Fire and Foam) drain valves to be opened, and drained. Seats to be clean prior boxing back. Integrity of the valves to be tested.\nAt present vessel has carried out Foam monitor valve renewal of No. 6 foam monitor and lapping and down filing of the seat has been conducted and same found operational. Isolation valves are to be attended to during the vessel's upcoming ballast passage.  Issue resolved.","2024-06-21T23:59:35","","Completed","2024-03-19T23:59:35","No","No","No","Internal"]
[null,null,null,32817,17722,"0_Mon Nov 27 2023 05:24:43 GMT+0800","2023-11-21T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Manifold hose saddled to be de-rusted and knife edges to be repaired. Once repaired Vertical Load test for rated 20T to be carried out. ","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","Equipment Related","","","","","Manifold hose saddled to be de-rusted and knife edges to be repaired. Once repaired Vertical Load test for rated 20T to be carried out. \nCarried out in dry dock and completed","2024-05-21T23:59:35","","Completed","2024-03-12T23:59:35","No","No","No","Internal"]
[null,null,null,32819,33325,"0_Mon Nov 27 2023 05:26:46 GMT+0800","2023-11-21T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Manifold drip trays to be hydro blasted.","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","Equipment Related","6.6","Medium","","","Manifold drip trays derusting in progress.","2024-07-21T23:59:35","","Completed","2024-03-18T23:59:35","No","No","Yes","Internal","Renewal of the manifold tray has been completed. Job to be closed."]
[null,null,null,32820,39493,"24_Mon Nov 27 2023 05:28:06 GMT+0800","2023-11-21T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Password required of the JRC radar installed IN ORDER TO ACCESS : File manager / Running hours record.","Navigation - RADAR","Navigation","Equipment Related","","","","","Password required of the JRC radar installed IN ORDER TO ACCESS : File manager / Running hours record.","2024-04-14T23:59:35","","Completed","2024-03-15T23:59:35","No","No","No","Internal"]
[null,null,null,32821,46898,"24_Mon Nov 27 2023 06:19:15 GMT+0800","2023-11-21T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Solenoid blocks inside VRCS Local solenoid boxes noted corroded","Deck - Machinery","Structural Condn. / WT integrity ","Equipment Related","8.11","Medium","","","Solenoid blocks inside VRCS Local solenoid boxes derusting & painting in progresss.\nCompleted in dry-dock","2024-05-21T23:59:35","","Completed","2024-03-15T23:59:35","No","No","No","Internal"]
[null,null,null,32822,28002,"24_Fri Dec 01 2023 13:30:18 GMT+0800","2023-11-21T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Navtex Printer alerts not legible. ","Navigation - GMDSS & Communication","Navigation","Equipment Related","4.7","High","","","Complete printer replaced with new received spare. In use.","2024-02-21T23:59:35","DBAU235075","Completed","2023-12-23T23:59:35","No","No","No","Internal"]
[null,null,null,32823,70152,"24_Mon Nov 27 2023 05:19:15 GMT+0800","2023-11-21T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Platform for the crane running wire winch along with railings eroded and wasted. Same are bolted in location : To be renewed and if permitted, welded in location","Deck - Machinery","Structural Condn. / WT integrity ","Equipment Related","8.50","Medium","","","Platform for the crane running wire winch along with railings eroded and wasted. Same are bolted in location : To be renewed and welded in location.\nCompleted in drydock","2024-02-21T23:59:35","","Completed","2024-03-18T23:59:35","No","No","No","Internal"]
[null,null,null,32833,74822,"0_Mon Nov 27 2023 05:29:35 GMT+0800","2023-11-21T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Purifier Room fwd side door not closing automatically\n","E/R - Purifier","Structural Condn. / WT integrity ","Equipment Related","5.35","Medium","","","Door closer adjusted. ","2024-02-21T23:59:35","NA","Completed","2023-11-24T23:59:35","No","No","No","Internal"]
[null,null,null,32836,39052,"0_Mon Nov 27 2023 05:23:12 GMT+0800","2023-11-21T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","1 no washing machine not operational ","Accommodation","General Appearance","Equipment Related","11.16","Low","","","Washing machine belt ordered & received in Stores at Singapore on 21-Nov-2023. Saem renewed & machine tried out. In use.","2024-02-21T23:59:35","","Completed","2023-11-25T23:59:35","No","No","No","Internal"]
[null,null,null,32835,86293,"24_Fri Dec 01 2023 13:39:33 GMT+0800","2023-11-22T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Explosion Proof light casing found cracked in Midship Store.","Elect. Mach. & Equip.","General Appearance","Equipment Related","11.11","Very High","","","Casing renewed with new spare.","2024-02-22T23:59:35","NA","Completed","2023-11-29T23:59:35","No","No","No","Internal"]
[null,null,null,32829,62322,"0_Fri Nov 17 2023 08:39:44 GMT+0800","2023-11-25T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Atmospheric Condenser Cooling Water Outlet U-bend stub piece leaking.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","U-bend removed & repaired the stub piece by welding. Installed back & in use.","2024-02-01T23:59:35","NA","Completed","2023-11-01T23:59:35","No","No","No","Internal"]
[null,null,null,34437,37976,"24_Tue Jan 02 2024 19:12:16 GMT+0800","2023-12-01T23:59:35","Observation","Ship Staff","Ship Staff Insp.","EGCS SW Feed Pump Discharge Line leak","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","EGCS SW feed pump discharge pipelines renewed in Drydock.","2024-03-01T23:59:35","NA","Completed","2024-03-16T23:59:35","No","No","No","Internal"]
[null,null,null,34439,95210,"0_Tue Jan 02 2024 19:15:21 GMT+0800","2023-12-01T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Sludge Pump found unable to transfer WO/Sludge to Incinerator WO Tank","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Pump opened up for inspection. Found the Stator competely damaged. The rotor also found with deep score marks. Renewed the rotor & stator with new onboard spares. Tried out & operating satisfactorily. RO raised for consumed spares.","2024-03-02T23:59:35","NA","Completed","2023-12-02T23:59:35","No","No","No","Internal"]
[null,null,null,34440,74499,"0_Tue Jan 02 2024 19:19:07 GMT+0800","2023-12-05T23:59:35","Observation","Ship Staff","Ship Staff Insp.","EGB Air Seal Fan operating with abnormal vibration.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Air Seal Fan Motor overhauled. Found bearings damaged. Same renewed with new spares. Fan boxed up, tried out & in use. ","2024-03-05T23:59:35","NA","Completed","2023-12-06T23:59:35","No","No","No","Internal"]
[null,null,null,34441,44392,"0_Tue Jan 02 2024 19:23:02 GMT+0800","2023-12-08T23:59:35","Observation","Ship Staff","Ship Staff Insp.","During ME LO Purifier operation, received “Purifier Abnormal Alarm”. The Purifier was re-started to check operation. Found the motor operating but the purifier not rotating.\n","E/R - Purifier","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","The motor was removed & the friction pads found worn out. Also observed unable to rotate the purifier via the friction boss. The crankcase was opened up for inspection & found contaminated with water. The vertical shaft also found with corrosion. The vertical shaft was removed & dismantled. Noticed the shaft with corrosion & pitting in the area where the water chamber sealing ring sits. This appears to be the cause of the water ingress.\nThe spring housing bearing also found damaged. The horizontal & vertical shaft renewed along with the bearings. All o-rings/gaskets renewed with new spares. Bowl routines also carried out & all spares renewed. tried out & in order.","2024-03-08T23:59:35","NA","Completed","2023-12-12T23:59:35","No","No","No","Internal"]
[null,null,null,34442,38071,"0_Tue Jan 02 2024 19:24:51 GMT+0800","2023-12-10T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Deck Seal Pumps Discharge Line T-Joint leaking.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Found pin hole leak from the weld seam. T-joint repaired by hotwork. Installed & in use.","2024-03-12T23:59:35","NA","Completed","2023-12-12T23:59:35","No","No","No","Internal"]
[null,null,null,34447,40865,"0_Tue Jan 02 2024 19:28:49 GMT+0800","2023-12-10T23:59:35","Observation","Ship Staff","Ship Staff Insp.","AE #1 Unit #2 & Unit #5 Fuel Pump leaking from the telltale hole.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Both fuel pumps renewed with overhauled spare. No leaks observed after replacement.","2024-03-13T23:59:35","NA","Completed","2023-12-13T23:59:35","No","No","No","Internal"]
[null,null,null,34446,57799,"0_Tue Jan 02 2024 19:32:22 GMT+0800","2023-12-14T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Sewage System not operational in Stbd Line.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","One pipe section found choked. Same removed & cleared manually. Installed back & system in use.","2024-03-14T23:59:35","NA","Completed","2023-12-14T23:59:35","No","No","No","Internal"]
[null,null,null,34443,12596,"0_Tue Jan 02 2024 19:37:09 GMT+0800","2023-12-18T23:59:35","Observation","Ship Staff","Ship Staff Insp.","FAULT alarm in Fire alarm Zone 11 (Zone 11 consist of engine casing and EGCS tower","Critical Equip.","Eng. / Strg. Comp.","Equipment Related","5.39","Very High","","","Upon inspection it was observed due to heavy rain and wind water ingress from nearby ventilation (in EGCS tower) to the detector SD 101. Detector SD 101 was immediately removed, cleaned using electronic circuit cleaner and dried. Ingress of water caused loop failure and caused Fault alarm (NO ANSWER) for all the detector and call point in Zone 11. After some time, Smoke detector 62 in Zone 14 was giving FAULT alarm (NO ANSWER) (Zone 14 in engine room) (Alarm photo attached). Upon further troubleshooting it was found Short Circuit Isolator for Zone 11 (Address 9) was damaged. (Photo attached). Vessel renewed the SCI (Salwico NS-SCI Part No. N11891) and observed all alarm resets but Fault alarm for SD 62 (Zone 14) & SD 101 (Zone 11) persist. Vessel renewed SD 62 (Zone 14) with a spare detector and fault alarm resets. Faulty sensor replaced with onboard spares & system restarted. Fault rectified.","2024-03-18T23:59:35","","Completed","2023-12-19T23:59:35","No","No","No","Internal"]
[null,null,null,34444,24291,"0_Tue Jan 02 2024 19:42:27 GMT+0800","2023-12-19T23:59:35","Observation","Ship Staff","Ship Staff Insp.","COP #1 Bottom Bearing Cooling line leaking during cargo discharge.","Cargo Mach.","Eng. / Strg. Comp.","Equipment Related","8.44","High","","","Cargo found leaking in the Pumproom. Line drained & renewed cooling line.","2024-03-19T23:59:35","NA","Completed","2023-12-19T23:59:35","No","No","No","Internal"]
[null,null,null,34438,54219,"0_Tue Jan 02 2024 19:47:50 GMT+0800","2023-12-20T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Sewage Vaccum pump found cutting in frequently.","E/R - Aux. Mach.,Accommodation","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Sewage vacuum line flap renewed and confirmed pump cutting off normally.","2024-03-20T23:59:35","DBAU230181","Completed","2024-03-25T23:59:35","No","No","No","Internal"]
[null,null,null,34445,71240,"0_Tue Jan 02 2024 19:45:53 GMT+0800","2023-12-20T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Sewage Vacuum Pump #1 found unable to create vaccum.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Pump dismantled & found motor coils damaged due to overheating. RO raised for new motor. Same installed & in use.","2024-03-20T23:59:35","DBAU230221","Completed","2023-12-27T23:59:35","No","No","No","Internal"]
[null,null,null,32346,64981,"0_Wed Nov 01 2023 09:43:44 GMT+0800","2024-03-20T23:59:35","Observation","Ship Staff","Ship Staff Insp.","EGCS SOx value in the analyser display is always showing 2 ppm.\nEGCS CO2 value in the analyser panel fluctuates between 0.9 to 1.6%.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.11","Medium","","","Alpha Laval technician attendend vessel on 04-July-2024 and carried out HOT-SWAP of gas analyzer. Analyzer initialization and calibration carried out, system found operational.","2024-06-30T23:59:35","DBAU245100","Completed","2024-07-04T23:59:35","No","No","Yes","Internal","Complete module is now in SINgapore and are planning to dispatch to Fujairah and planning to arrange AL SE to attend and install."]
[null,null,null,34865,21624,"24_Tue Apr 02 2024 18:47:49 GMT+0800","2024-03-23T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Spare Main Engine Piston to be overhauled and kept as standby. ","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Main engine spare piston overhauled and kept as standby.","2024-04-15T23:59:35","","Completed","2024-05-18T23:59:35","No","No","No","Internal"]
[null,null,null,34866,99571,"24_Tue Apr 02 2024 23:58:44 GMT+0800","2024-03-23T23:59:35","Breakdown","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Several gratings for walkways on the deck to be renewed as few found to be rusted.  ","Deck - Pipe / Fittings","ISM Related","Equipment Related","","","","","To be carried out.\nCompleted on 05.05.2024","2024-04-23T23:59:35","","Completed","2024-05-05T23:59:35","No","No","No","Internal"]
[null,null,null,34867,17882,"24_Wed Apr 03 2024 00:09:36 GMT+0800","2024-03-23T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Aft facing light fitting on the paint locker platform is in not very good condition. Support to be renewed.","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","Equipment Related","","","","","Aft facing light fitting support renewed.","2024-05-30T23:59:35","","Completed","2024-04-22T23:59:35","No","No","No","Internal"]
[null,null,null,34868,43666,"24_Wed Apr 03 2024 00:11:18 GMT+0800","2024-03-23T23:59:35","Breakdown","Owner / Marine / Tech. Suptd.","Suptd. Insp.","IG main line pressure gauge in the Pump room not working. To be renewed. ","Cargo Mach.","Cargo / Ballast Systems","Industry Issue","","","","","Gauge replaced with working gauge.","2024-04-08T23:59:35","","Completed","2024-04-15T23:59:35","No","No","No","Internal"]
[null,null,null,34869,15599,"24_Wed Apr 03 2024 00:12:36 GMT+0800","2024-03-23T23:59:35","Breakdown,Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Telephone in the bosun store in damaged and needs to be renewed.","Elect. Mach. & Equip.","Communication","Equipment Related","","","","","Telephone renewed.","2024-04-23T23:59:35","","Completed","2024-05-06T23:59:35","No","No","No","Internal","Spares will be supplied in Singapore"]
[null,null,null,34870,68816,"24_Tue Apr 02 2024 18:56:51 GMT+0800","2024-03-23T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","EGE Exhaust gas IN/OUT diff gauge in the ECR console found not working \t","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","EGE Exhaust gas IN/OUT diff pressure transmitter line opened up and cleared. now working satisfactory.","2024-04-21T23:59:35","","Completed","2024-05-15T23:59:35","No","No","No","Internal"]
[null,null,null,34871,47773,"0_Wed Apr 03 2024 00:07:09 GMT+0800","2024-03-23T23:59:35","Breakdown,Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Paint locker natural vent louvre needs to be derusted. ","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","Equipment Related","","","","","to be carried out.\nCOMPLETED ON 04.05.2024","2024-04-23T23:59:35","","Completed","2024-05-04T23:59:35","No","No","No","Internal"]
[null,null,null,34873,72523,"24_Tue Apr 02 2024 19:29:43 GMT+0800","2024-03-23T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Several seal pots in the Engine room found empty. To be filled with water. ","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","All  seal pots in engineroom filled with water.","2024-04-07T23:59:35","","Completed","2024-03-30T23:59:35","No","No","No","Internal"]
[null,null,null,34874,82214,"24_Tue Apr 02 2024 19:23:48 GMT+0800","2024-03-23T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","IG scrubber tower high level switch found damaged. To be renewed. ","Cargo Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","IG scrubber tower high level switch renewed.","2024-03-30T23:59:35","","Completed","2024-03-25T23:59:35","No","No","No","Internal"]
[null,null,null,34876,52155,"24_Tue Apr 02 2024 19:09:02 GMT+0800","2024-03-23T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Main Engine Fuel testing room needs to be squared up and very untidy. ","E/R - Main Engine,E/R - Aux. Engine","Eng. / Strg. Comp.","Behaviour Based","10.32","Very High","","","Main Engine Fuel testing room squared up and cleaned.","2024-04-21T23:59:35","","Completed","2024-04-03T23:59:35","No","No","No","Internal"]
[null,null,null,34872,85193,"24_Tue Apr 02 2024 19:17:05 GMT+0800","2024-04-01T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Few insulation mats in front of 440V starter panels found damaged. Needs to be renewed. ","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.24","Low","","","Damaged insulation mats renewed.","2024-04-15T23:59:35","","Completed","2024-04-02T23:59:35","No","No","No","Internal"]
[null,null,null,34875,94632,"24_Tue Apr 02 2024 19:00:32 GMT+0800","2024-04-01T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Main Engine Aft TC grit washing hopper found sheered off from base. This needs to be welded in place. ","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Main Engine Aft TC grit washing hopper removed from place and repaired. Same fixed back.","2024-04-07T23:59:35","","Completed","2024-04-01T23:59:35","No","No","No","Internal"]
[null,null,null,34893,28775,"24_Fri Apr 12 2024 16:58:36 GMT+0800","2024-04-11T23:59:35","Defect","Ship Staff","Ship Staff Insp.","S band radar showing ' AZI error ' continuously . ","Navigation - RADAR","Navigation","Equipment Related","","","","","Office informed and troubleshooting as per instructions from office in progress \nProblem sorted by ETO and health check carried out by shore technitian and all found in order.","2024-07-12T23:59:35","","Completed","2024-04-30T23:59:35","No","No","No","Internal"]
[null,null,null,34894,64623,"24_Fri Apr 12 2024 17:03:29 GMT+0800","2024-04-12T23:59:35","Defect,Guarantee Claim","Ship Staff","Ship Staff Insp.","Newly supplied hydroblaster not operational within 2 days initial operational. The dump gun of the blaster found continuously leaking water hence unable to build pressure sufficient for hydroblasting ","Deck - Machinery","General Appearance","Equipment Related","","","","","Service engineer attended vessel on 4th July 2024 and rectified the fault. Hydroblaster operation tried out and found satisfactory.","2024-07-12T23:59:35","","Completed","2024-07-04T23:59:35","No","No","No","Internal"]
[null,null,null,36224,87324,"24_Sat Jun 22 2024 23:03:28 GMT+0800","2024-04-12T23:59:35","Observation","Ship Staff","Ship Staff Insp.","COT 5C valve CL-245  indication closing after being fully open","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","Valve issue has been rectified. The indication did not come to open position when the valve is fully open. The indication unit for valve CL-245 was dismantled and troubleshooting carried out. Observed issue with the potentiometer as it was showing open line while the indication was more than 70% open. No spare potentiometer was found on board. Old valves were disassembled and one potentiometer was found in working condition. Same was installed and tried out. Found issue with the setting value as it was showing 15% open while the valve was closed completely. Again, removed the valve and calibrated the potentiometer as per the position. Tried out and found working satisfactory","2024-07-12T23:59:35","","Completed","2024-05-10T23:59:35","No","No","No","Internal"]
[null,null,null,36225,29826,"24_Sat Jun 22 2024 23:15:32 GMT+0800","2024-04-12T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Bottom x-over valve CL231 not showing O/S indication","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","Valve No. 231 in VRCS cargo console system in the CCR was reported not showing correct indication in the CCC panel. Observed that although the signal constantly shows closed the valve was opening to a max of 70% and closing a maximum of 30% and during operation was causing abnormal sound. The indication unit was dismantled and troubleshooting carried out. Observed that the oval gear fitting was incorrect which prevented valve from opening or closing fully. Further investigation showed a driving gear tooth was damaged. Old discarded valve was opened and scavenged a working gear and replaced it. Fitted back full unit and tried out. Found working correctly. Now the indication for open and closed are also functional.","2024-07-12T23:59:35","","Completed","2024-05-13T23:59:35","No","No","No","Internal"]
[null,null,null,36226,75173,"24_Sat Jun 22 2024 23:57:27 GMT+0800","2024-04-12T23:59:35","Defect","Ship Staff","Ship Staff Insp.","5S WBT stripper valve BA 419 not operational from CCR. ","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","Vessel is carrying out the trobleshooting for the same and will revert with details once completed.\nVessel opened the lock nut for the valve in the Solenoid VRCS cabinet \n & found that the needle valve was shut and preventing the valve from operating remotely from CCR. The needle valve was throttled open and valve operated from CCR. Found that the valve was operating as per command given from CCR. Lock nut was secured and tried out the valve operation from CCR 2-3 times and found working satisfactorily.","2024-07-12T23:59:35","","Completed","2024-06-21T23:59:35","No","No","No","Internal"]
[null,null,null,32349,20821,"0_Wed Nov 01 2023 09:52:40 GMT+0800","2024-04-15T23:59:35","Observation","Ship Staff","Ship Staff Insp.","BWTS TRO #1 Signal failure alarm activated.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","6.21","High","","","TROUBLESHOOTING CARRIED OUT AS PER MAKER AND RECTIFIED THE SIGNAL FAILURE ALARM. ","2024-06-30T23:59:35","","Completed","2024-06-26T23:59:35","No","No","Yes","Internal","Please resend the email for this issue."]
[null,null,null,35694,78090,"24_Tue May 21 2024 15:44:50 GMT+0800","2024-05-16T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Action item -VRCS hydraulic pump suction filters and filters and all line filters at 3 monthly interval - PMS job to be created.","Cargo Mach.","Eng. / Strg. Comp.","Equipment Related","8.11","Medium","","","PMS job created.","2024-06-15T23:59:35","","Completed","2024-06-14T23:59:35","No","No","No","Internal","Implemented. Can be closed."]
[null,null,null,35695,62201,"24_Tue May 21 2024 15:58:02 GMT+0800","2024-05-16T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Action item-LO sample to be drawn from valve box on deck instead of sample from tank - LO sample to be drawn from valve box on deck instead of sample from tank - PMS job description to be amended","Cargo Mach.","Eng. / Strg. Comp.","Equipment Related","8.11","Medium","","","CRF raised-PMS job description has been amended","2024-06-15T23:59:35","","Completed","2024-05-15T23:59:35","No","No","No","Internal","CRF has been implemented."]
[null,null,null,35696,46599,"24_Tue May 21 2024 15:40:45 GMT+0800","2024-05-16T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Action item-All dirty oil drums in steering gear room, waiting for disposal, to be properly identified and marked. All fleet vessels to be notified.","Cargo Mach.","Eng. / Strg. Comp.","Equipment Related","8.11","Medium","","","All oil drums identified and marked as \"IN USE/DIRTY OIL/EMPTY\".","2024-05-30T23:59:35","","Completed","2024-05-19T23:59:35","No","No","No","Internal"]
[null,null,null,35697,31735,"24_Tue May 21 2024 15:54:54 GMT+0800","2024-05-16T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Only dedicated pipe and pump to be used for transferring oil from new oil drum to Hydraulic oil tank. All fleet vessels to be notified.","Cargo Mach.","Eng. / Strg. Comp.","Equipment Related","8.11","Medium","","","Dedicated pump and pipe kept near VRCS tank and tagged \" USE ONLY FOR VRCS OIL FILLING\"","2024-05-30T23:59:35","","Completed","2024-05-18T23:59:35","No","No","No","Internal"]
[null,null,null,35698,68498,"24_Tue May 21 2024 16:03:38 GMT+0800","2024-05-16T23:59:35","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Action item- Portable filter equipment to be supplied for hydraulic oil filtration and cleanliness.","Cargo Mach.","Eng. / Strg. Comp.","Equipment Related","8.11","Medium","","","Portable filter equipment received on 18/04/2024 ","2024-05-30T23:59:35","","Completed","2024-05-16T23:59:35","No","No","No","Internal"]
[null,null,null,35699,60901,"24_Tue May 21 2024 16:16:38 GMT+0800","2024-05-16T23:59:35","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Action item-New filters for pumps suction, line filters on deck and line filter in VRCS hydraulic room to be supplied from Maker (Nanakita).","Cargo Mach.","Eng. / Strg. Comp.","Equipment Related","8.11","Medium","","","New filters kept in the spare room is supplied from the maker, and Filter RO to be raised only from the maker, same posted in the spare locker in VRCS section.","2024-05-30T23:59:35","","Completed","2024-05-20T23:59:35","No","No","No","Internal"]
[null,null,null,35700,48365,"24_Tue May 21 2024 15:28:48 GMT+0800","2024-05-16T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Action items-C/E to ensure only the cleaned and correct grade oil is used to top up the system. A ‘placard’ to this effect to be displayed in VRCS room to alert the crew to take C/E’s permission to top up oil. All fleet vessels to be notified.","Cargo Mach.","Eng. / Strg. Comp.","Inappropriate Procedure","8.11","Medium","","","Posted placard- do not fill oil without chief engineer's permission. near the filling connection of VRCS tank.","2024-05-31T23:59:35","","Completed","2024-05-18T23:59:35","No","No","No","Internal"]
[null,null,null,36220,22191,"24_Wed Jun 26 2024 09:42:04 GMT+0800","2024-05-28T23:59:35","Observation","Ship Staff","Ship Staff Insp.","#2 Reefer compressor control panel magnetic contactor found faulty and system is not operational.","Accommodation","General Appearance","Equipment Related","10.38","Medium","","","Renewed the faulty magnetic contactor and tried out. #2 reefer operation found satisfactory.","2024-08-14T23:59:35","DBAU240111","Completed","2024-07-15T23:59:35","No","No","No","Internal"]
[null,null,null,36214,30713,"24_Sat Jun 15 2024 21:17:55 GMT+0800","2024-05-30T23:59:35","Observation","Ship Staff","Ship Staff Insp.","ME Fuel Valve Testing Device Trouble.","E/R - Main Engine,Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Fault was identified with the pressure relief valve...after few operations, the relief valve did not sit properly, resulting in pressure not being built up. Relief valve overhauled. Testing device tried out several times and found to be working satisfactory","2024-08-15T23:59:35","","Completed","2024-07-17T23:59:35","No","No","No","Internal"]
[null,null,null,36213,20845,"24_Fri Jun 14 2024 22:08:08 GMT+0800","2024-06-06T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Accommodation gas detection system #2 HC Sensor faulty","Elect. Mach. & Equip.","Safety / LSA / FFA","Equipment Related","8.41","Medium","","","New spare received and replaced the defective sensor, calibrated new sensor and system restarted. Gas detection system tried out and found in order.","2024-08-06T23:59:35","DBAU245103","Completed","2024-06-29T23:59:35","No","No","No","Internal"]
[null,null,null,36211,77438,"24_Thu Jun 27 2024 19:56:23 GMT+0800","2024-06-23T23:59:35","Observation","Ship Staff","Ship Staff Insp.","2 nos. tank vent heads found corroded","Hull & Tanks","General Appearance","External Factors","11.7","High","","","Repair work of damaged vent heads carried out.","2024-09-22T23:59:35","","Completed","2024-07-15T23:59:35","No","No","No","Internal","As discussed please order spares complete head and we will supply at the earliest."]
[null,null,null,36513,62157,"24_Wed Jul 17 2024 13:12:42 GMT+0800","2024-07-04T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Main Air Compressor no 1 sump oil was found emulsified. To be investigated.","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","MAC no.1, 1000 hrs routines carried out. All 4 stages valve renewed, LO filter renewed, sump oil renewed, leak test done and crankcase inspection carried out. Compressor tried out, found working satisfactory.","2024-07-19T23:59:35","","Completed","2024-07-08T23:59:35","No","No","No","Internal"]
[null,null,null,36514,62611,"24_Wed Jul 17 2024 13:23:20 GMT+0800","2024-07-04T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Speaker for Light column at the aft of Aux Engines is not functioning. ","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.37","Medium","","","Renewed the faulty PCB and treid out.","2024-08-04T23:59:35","","Completed","2024-07-17T23:59:35","No","No","No","Internal"]
[null,null,null,36515,47474,"24_Wed Jul 17 2024 13:39:28 GMT+0800","2024-07-04T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Paint burn marks from DD are still visible in the emergency escape trunk. ","Miscellaneous","General Appearance","External Factors","11.1","High","","","In emergency escape trunk burn marks buffing and painting carried out.","2024-08-04T23:59:35","","Completed","2024-07-17T23:59:35","No","No","No","Internal"]
[null,null,null,36510,99023,"24_Tue Jul 16 2024 13:17:42 GMT+0800","2024-07-11T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Port side manifold drip tray pipe support stand found holed during routine maintenance.","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","Equipment Related","11.5","Medium","","","Temporary repairs have been carried out on the same ","2024-10-10T23:59:35","","Completed","2024-07-15T23:59:35","No","No","No","Internal"]
[null,null,null,null,43351,"24_Tue Jul 16 2024 21:00:18 GMT+0800","2024-07-04T08:00:00","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Several fire doors in the Accommodation were found left in an OPEN position secured with rope etc. This is a serious fire and safety hazard. \t","LSA / FFA,Miscellaneous","Safety / LSA / FFA","Human Error","5.1","Very High","","","Training given to all staff and all fire doors being kept shut ","2024-07-16T08:00:00","","Completed","2024-07-16T08:00:00","No","No","No","Internal"]
[null,null,null,null,14975,"0_Tue Jul 16 2024 21:06:18 GMT+0800","2024-07-04T08:00:00","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Several ship staff were found not using covers on the walkie-talkies. This is the biggest cause of damage. ","Critical Equip.","Crew Management","Behaviour Based","5.5","Low","","","Training given to all staff and told to use walkie talkie covers at all times.","2024-07-16T08:00:00","","Completed","2024-07-16T08:00:00","No","No","No","Internal"]
[null,null,null,null,70241,"24_Wed Jul 17 2024 12:52:39 GMT+0800","2024-07-04T08:00:00","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","HFO 2S bunker tank vent head found rusted.","Hull & Tanks","General Appearance","External Factors","11.7","High","","","HFO 2S bunker tank vent head derusted and maintenance carried out.  ","2024-07-19T08:00:00","","Completed","2024-07-18T08:00:00","No","No","No","Internal"]
[null,null,null,null,18494,"24_Tue Jul 16 2024 21:02:27 GMT+0800","2024-07-04T08:00:00","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Galley Cooking Oil can color code to be corrected. Refer to the Garbage Management plan for the correct color code. ","Miscellaneous","MARPOL Related","External Factors","6.20","Medium","","","To be carried out.\nColour coding carried out as per GMP","2024-08-04T08:00:00","","Completed","2024-07-27T08:00:00","No","No","No","Internal"]
[null,null,null,null,10580,"0_Tue Jul 16 2024 21:09:09 GMT+0800","2024-07-04T08:00:00","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Steering Gear room aft entrance door securing latch is damaged. ","Deck - Pipe / Fittings","Eng. / Strg. Comp.","Equipment Related","11.6","Medium","","","Aft steering entrance door hook is in place and operational","2024-08-04T08:00:00","","Completed","2024-07-28T08:00:00","No","No","No","Internal"]
[null,null,null,null,10075,"0_Tue Jul 16 2024 21:11:10 GMT+0800","2024-07-04T08:00:00","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Safety latch of the Chain block kept in the forward locker was found damaged. To be renewed. ","Deck - Pipe / Fittings","ISM Related","Equipment Related","5.11","Low","","","Safety Latch has been attached","2024-08-04T08:00:00","","Completed","2024-07-25T08:00:00","No","No","No","Internal"]
[null,null,null,null,62125,"24_Tue Jul 16 2024 21:13:05 GMT+0800","2024-07-04T08:00:00","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","All mooring rollers in the forward section were found and not free to move. ","Deck - Machinery","Mooring","Equipment Related","9.18","Low","","","To free up mooring rollers.\nMooring rollers have been freed up. after removing the rollers from base and carrying out maintenance on them.","2024-09-04T08:00:00","","Completed","2024-07-19T08:00:00","No","No","No","Internal"]
[null,null,null,null,12686,"24_Wed Jul 17 2024 13:30:18 GMT+0800","2024-07-04T08:00:00","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Both AC compressor coupling shaft covers do not provide adequate cover. Protection cover to be extended to ensure safety.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.27","Medium","","","Both AC compressor coupling shaft covers modified and fixed back.","2024-08-04T08:00:00","","Completed","2024-07-29T08:00:00","No","No","No","Internal"]
[null,null,null,null,59286,"24_Sat Jun 22 2024 23:23:07 GMT+0800","2024-06-22T08:00:00","Observation","Ship Staff","Ship Staff Insp.","COT 2 S valve CL-207 operation slow. ","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.11","Medium","","","At present vessel is monitoring the valve and ensuring that its fully open or closed. Vessel will attend to this valve during the next ballast passage. Suspect the oil supply to the valve is throttled. \nVessel adjusted the needle valve after opening the lock nut and increased the oil flow and the speed of the valve  to operate faster. same was noticed to be closing in required time.","2024-09-22T08:00:00","","Completed","2024-07-19T08:00:00","No","No","No","Internal"]
[null,null,null,null,62407,"24_Tue Jul 16 2024 13:20:31 GMT+0800","2024-07-16T08:00:00","Defect","Ship Staff","Ship Staff Insp.","No sampling ports for ballast tanks, apart from FPK and APK","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","","","","","Vessel has received fabrication material for the same and has already prepared sampling ports for 5P, 5S, 4S and 3S WBT's. Rest are planned to be completed asap.\nAll ballast manholes fabrication for sampling portshas been completed.","2024-10-15T08:00:00","","Completed","2024-08-02T08:00:00","No","No","No","Internal","Vessel to complete before arrival Discharge port."]
[null,null,null,null,95204,"24_Tue Jul 16 2024 20:03:46 GMT+0800","2024-07-11T08:00:00","Observation","Ship Staff","Ship Staff Insp.","Incinerator HMI panel switching off intermittently.","Critical Equip.","MARPOL Related","Equipment Related","10.32","Very High","","","Temporary PSU added and HMI working satisfactorily.","2024-09-11T08:00:00","","Completed","2024-07-27T08:00:00","No","No","No","Internal"]

{"sheet":"Calc","index":2,"n_rows":28,"n_cols":12,"rows_kept":28,"cut":false,"hidden":true,"merged":[]}
["Def_type","Def_cause","Equipments","VIQrefno","Observer_code"]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,"Dim itemSele As Long"]
[null,null,null,null,null,null,null,null,null,null,null,"   dim startRow as integer"]
[null,null,null,null,null,null,null,null,null,null,null,"   startRow=1"]
[null,null,null,null,null,null,null,null,null,null,null,"        For itemSele = 0 To ListBox1.ListCount - 1"]
[null,null,null,null,null,null,null,null,null,null,null,"        If ListBox1.Selected(itemSele) = True Then"]
[null,null,null,null,null,null,null,null,null,null,null,"        Worksheets(\"WorksheetName\").Range(\"A\" & startRow).Value = ListBox1.List(itemSele)"]
[null,null,null,null,null,null,null,null,null,null,null,"        startRow = startRow + 1"]
[null,null,null,null,null,null,null,null,null,null,null,"        End If"]
[null,null,null,null,null,null,null,null,null,null,null,"        Next"]
[null,null,null,null,null,null,null,null,null,null,null,"Dim LastRowA As String"]
[null,null,null,null,null,null,null,null,null,null,null,"        Dim itemSele As Long"]
[null,null,null,null,null,null,null,null,null,null,null,"       Dim startRow as integer"]
[null,null,null,null,null,null,null,null,null,null,null,"        LastRowA = ActiveSheet.Cells(Rows.count, \"A\").End(xlUp).row"]
[null,null,null,null,null,null,null,null,null,null,null,"        startQue = 0"]
[null,null,null,null,null,null,null,null,null,null,null,"        For itemSele = 0 To ListBox1.ListCount - 1"]
[null,null,null,null,null,null,null,null,null,null,null,"        For startRow = 1 To LastRowA"]
[null,null,null,null,null,null,null,null,null,null,null,"        If Worksheets(\"WorksheetName\").Range(\"A\" & startRow).Value = ListBox1.List(itemSele) Then"]
[null,null,null,null,null,null,null,null,null,null,null,"        ListBox1.Selected(itemSele) = True"]
[null,null,null,null,null,null,null,null,null,null,null,"        Exit For"]
[null,null,null,null,null,null,null,null,null,null,null,"        End If"]
[null,null,null,null,null,null,null,null,null,null,null,"        Next j"]
[null,null,null,null,null,null,null,null,null,null,null,"        Next"]
[null,null,null,null,null,null,null,null,null,null,null,"        End If"]

{"sheet":"Areaofobs","index":3,"n_rows":17,"n_cols":2,"rows_kept":17,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Cargo / Ballast Systems",11]
["Cert. & Docu.",2]
["Communication",6]
["Crew Management",3]
["Emgcy. Systems",13]
["Eng. / Strg. Comp.",14]
["General Appearance",15]
["Ice Opns.",17]
["ISM Related",7]
["ISPS Related",10]
["MARPOL Related",9]
["MLC Related",4]
["Mooring",12]
["Navigation",5]
["Safety / LSA / FFA",8]
["Structural Condn. / WT integrity ",16]

{"sheet":"Vessel_type","index":4,"n_rows":1,"n_cols":2,"rows_kept":1,"cut":false,"hidden":true,"merged":[]}
["Vessel_type","ID"]

{"sheet":"Deficiency_type","index":5,"n_rows":8,"n_cols":3,"rows_kept":8,"cut":false,"hidden":true,"merged":[]}
["TITLE","Type of deficiency_description","ID"]
["Breakdown",null,6]
["Critical Equipment",null,4]
["Defect",null,1]
["Guarantee Claim",null,8]
["Non Conformity",null,2]
["Observation",null,3]
["Other",null,7]

{"sheet":"VIQrefno","index":6,"n_rows":427,"n_cols":3,"rows_kept":427,"cut":false,"hidden":true,"merged":[]}
["VIQ_ref_no","Risk Value of observation","ID"]
["1.1","Low",8243]
["1.10","Low",8252]
["1.11","Low",8253]
["1.12","Low",8254]
["1.13","Low",8255]
["1.14","Low",8256]
["1.15","Low",8257]
["1.16","Low",8259]
["1.17","Low",8260]
["1.18","Low",8261]
["1.19","Low",8262]
["1.2","Low",8244]
["1.20","Low",8263]
["1.21","Low",8265]
["1.22","Low",8266]
["1.23","Low",8267]
["1.24","Low",8268]
["1.25","Low",8269]
["1.26","Low",8270]
["1.3","Low",8245]
["1.4","Low",8246]
["1.5","Low",8247]
["1.6","Low",8248]
["1.7","Low",8249]
["1.8","Low",8250]
["1.9","Low",8251]
["1.99","High",11258]
["10.1","Medium",8461]
["10.10","High",8470]
["10.11","Medium",8471]
["10.12","Very High",8472]
["10.13","Very High",8473]
["10.14","Medium",8474]
["10.15","Low",8475]
["10.16","Very High",8476]
["10.17","Very High",8477]
["10.18","High",8478]
["10.19","Very High",8479]
["10.2","Low",8462]
["10.20","High",8480]
["10.21","Medium",8481]
["10.22","Low",8482]
["10.23","Medium",8483]
["10.24","Low",8484]
["10.25","Very High",8485]
["10.26","High",8486]
["10.27","Medium",8487]
["10.28","Low",8488]
["10.29","Medium",8489]
["10.3","Medium",8463]
["10.30","High",8490]
["10.31","Very High",8491]
["10.32","Very High",8492]
["10.33","High",8493]
["10.34","High",8494]
["10.35","Very High",8495]
["10.36","Very High",8496]
["10.37","Medium",8497]
["10.38","Medium",8498]
["10.39","High",8499]
["10.4","High",8464]
["10.40","Medium",8500]
["10.41","Medium",8501]
["10.42","Medium",8502]
["10.43","Medium",8503]
["10.44","Medium",8504]
["10.45","Very High",8505]
["10.46","High",8506]
["10.47","Medium",8507]
["10.48","High",8508]
["10.49","Medium",8509]
["10.5","Low",8465]
["10.50","High",8510]
["10.51","Low",8511]
["10.52","Medium",8512]
["10.53","Medium",8513]
["10.54","High",8514]
["10.55","Low",8515]
["10.6","Very High",8466]
["10.7","Medium",8467]
["10.8","Medium",8468]
["10.9","Medium",8469]
["10.99","High",8516]
["11.1","High",8420]
["11.10","Medium",8429]
["11.11","Very High",8430]
["11.12","Low",8431]
["11.13","Low",8432]
["11.14","Medium",8433]
["11.15","Low",8434]
["11.16","Low",8435]
["11.17","Low",8436]
["11.2","Medium",8421]
["11.3","Medium",8422]
["11.4","Very High",8423]
["11.5","Medium",8424]
["11.6","Medium",8425]
["11.7","High",8426]
["11.8","Low",8427]
["11.9","Low",8428]
["11.99","High",8437]
["12.1","High",8438]
["12.10","High",8448]
["12.11","High",8449]
["12.12","High",8450]
["12.13","High",8451]
["12.14","High",8452]
["12.15","High",8453]
["12.16","High",8454]
["12.17","High",8455]
["12.18","High",8456]
["12.19","High",8457]
["12.2","High",8439]
["12.20","High",8458]
["12.21","High",8459]
["12.3","High",8441]
["12.4","High",8442]
["12.5","High",8443]
["12.6","High",8444]
["12.7","High",8445]
["12.8","High",8446]
["12.9","High",8447]
["12.99","High",8460]
["2.1","Very High",8296]
["2.1.9","Very High",11259]
["2.10","Medium",8304]
["2.11","Medium",8305]
["2.12","Low",8306]
["2.13","Low",8307]
["2.14","Low",8308]
["2.15","Low",8309]
["2.16","Medium",8310]
["2.2","Medium",8297]
["2.3","High",8295]
["2.4","Medium",8298]
["2.5","Medium",8299]
["2.6","Low",8300]
["2.7","High",8301]
["2.8","High",8302]
["2.9","Medium",8303]
["2.99","High",8311]
["3.1","High",8312]
["3.2","Very High",8313]
["3.3","High",8314]
["3.4","Low",8294]
["3.5","Medium",8315]
["3.6","High",8316]
["3.7","Very High",8317]
["3.8","Very High",8318]
["3.99","High",8319]
["4.1","High",8320]
["4.10","High",8329]
["4.11","Medium",8330]
["4.12","Very High",8331]
["4.13","Very High",8332]
["4.14","Very High",8333]
["4.15","Very High",8334]
["4.16","Very High",8335]
["4.17","Very High",8336]
["4.18","Very High",8337]
["4.19","Low",8338]
["4.2","Medium",8321]
["4.20","Very High",8339]
["4.21","High",8340]
["4.22","Low",8341]
["4.23","High",8342]
["4.24","High",8343]
["4.25","Low",8344]
["4.26","Low",8345]
["4.27","High",8346]
["4.3","Medium",8322]
["4.4","High",8323]
["4.5","Very High",8324]
["4.6","Medium",8325]
["4.7","High",8326]
["4.8","Medium",8327]
["4.9","Medium",8328]
["4.99","High",8347]
["5.1","Very High",8517]
["5.10","High",8526]
["5.11","Low",8527]
["5.12","Medium",8528]
["5.13","High",8529]
["5.14","Very High",8530]
["5.15","Medium",8531]
["5.16","Very High",8532]
["5.17","Very High",8533]
["5.18","High",8534]
["5.19","Medium",8535]
["5.2","Very High",8518]
["5.20","Medium",8536]
["5.21","Medium",8537]
["5.22","High",8539]
["5.23","Very High",8540]
["5.24","Very High",8541]
["5.25","Medium",8542]
["5.26","Medium",8543]
["5.27","Medium",8544]
["5.28","Very High",8545]
["5.29","High",8546]
["5.3","Low",8519]
["5.30","High",8547]
["5.31","High",8548]
["5.32","High",8549]
["5.33","High",8550]
["5.34","Low",8551]
["5.35","Medium",8552]
["5.36","Low",8553]
["5.37","Low",8554]
["5.38","High",8555]
["5.39","Very High",8556]
["5.4","High",8520]
["5.40","Very High",8557]
["5.41","Very High",8558]
["5.42","Medium",8559]
["5.43","High",8560]
["5.44","High",8561]
["5.45","Medium",8564]
["5.46","Medium",8565]
["5.47","Medium",8566]
["5.48","Medium",8567]
["5.5","Low",8521]
["5.6","Low",8522]
["5.7","Medium",8523]
["5.8","Medium",8524]
["5.9","Very High",8525]
["5.99","High",8568]
["6.1","Medium",8348]
["6.10","Low",8357]
["6.11","High",8358]
["6.12","Medium",8359]
["6.13","Low",8360]
["6.14","High",8361]
["6.15","High",8362]
["6.16","Very High",8363]
["6.17","Very High",8364]
["6.18","Medium",8365]
["6.19","Low",8366]
["6.2","High",8349]
["6.20","Medium",8367]
["6.21","High",8368]
["6.22","Medium",8369]
["6.3","Low",8350]
["6.4","High",8351]
["6.5","Medium",8352]
["6.6","Medium",8353]
["6.7","High",8354]
["6.8","High",8355]
["6.9","Low",8356]
["6.99","High",8370]
["7.1","High",8371]
["7.10","High",8380]
["7.11","High",8381]
["7.12","High",8382]
["7.13","Medium",8383]
["7.14","Medium",8384]
["7.15","High",8385]
["7.16","High",8386]
["7.17","High",8387]
["7.2","High",8372]
["7.3","Low",8373]
["7.4","Low",8374]
["7.5","Low",8375]
["7.6","Medium",8376]
["7.7","Low",8377]
["7.8","High",8378]
["7.9","High",8379]
["7.99","High",8388]
["8.1","Very High",8569]
["8.10","Very High",8578]
["8.100","Low",11227]
["8.101","Medium",11228]
["8.102","Low",11229]
["8.103","Low",11230]
["8.104","Low",11231]
["8.105","Medium",11232]
["8.106","Medium",11233]
["8.107","Low",11234]
["8.108","High",11235]
["8.109","Very High",11236]
["8.11","Medium",8579]
["8.110","High",11237]
["8.111","Medium",11238]
["8.112","High",11239]
["8.113","Medium",11240]
["8.114","Low",11241]
["8.115","High",11242]
["8.116","Medium",11243]
["8.117","Medium",11244]
["8.118","Medium",11245]
["8.119","High",11246]
["8.12","Medium",8580]
["8.120","High",11247]
["8.121","Medium",11248]
["8.122","High",11249]
["8.123","High",11250]
["8.124","Low",11251]
["8.125","High",11252]
["8.126","Medium",11253]
["8.127","Medium",11254]
["8.13","Medium",8581]
["8.14","Very High",8582]
["8.15","High",8583]
["8.16","Very High",8584]
["8.17","Low",8585]
["8.18","High",8586]
["8.19","High",8587]
["8.199","High",11255]
["8.2","Medium",8570]
["8.20","Medium",8588]
["8.21","High",8589]
["8.22","Very High",8590]
["8.23","Medium",8591]
["8.24","Medium",8592]
["8.25","Very High",8593]
["8.26","High",8594]
["8.27","Medium",8595]
["8.28","Medium",8596]
["8.29","High",8598]
["8.3","Very High",8571]
["8.30","High",8599]
["8.31","High",8600]
["8.32","Low",8601]
["8.33","Medium",8602]
["8.34","High",8603]
["8.35","Medium",8604]
["8.36","Medium",8605]
["8.37","High",8607]
["8.38","Medium",8608]
["8.39","Medium",8609]
["8.4","Medium",8572]
["8.40","High",8610]
["8.41","Medium",8611]
["8.42","Medium",8612]
["8.43","Very High",8613]
["8.44","High",8615]
["8.45","High",8616]
["8.46","Very High",8617]
["8.47","Very High",8618]
["8.48","Medium",8619]
["8.49","High",8620]
["8.5","Very High",8573]
["8.50","Medium",8621]
["8.51","Low",8622]
["8.52","Low",8623]
["8.53","Low",8624]
["8.54","High",8625]
["8.55","Low",11182]
["8.56","Medium",11183]
["8.57","Medium",11184]
["8.58","High",11185]
["8.59","High",11186]
["8.6","Medium",8574]
["8.60","High",11187]
["8.61","Medium",11188]
["8.62","Very High",11189]
["8.63","High",11190]
["8.64","Medium",11191]
["8.65","Low",11192]
["8.66","High",11193]
["8.67","High",11194]
["8.68","High",11195]
["8.69","Medium",11196]
["8.7","High",8575]
["8.70","Medium",11197]
["8.71","Very High",11198]
["8.72","Medium",11199]
["8.73","Medium",11200]
["8.74","High",11201]
["8.75","Medium",11202]
["8.76","Medium",11203]
["8.77","Medium",11204]
["8.78","Medium",11205]
["8.79","Medium",11206]
["8.8","Medium",8576]
["8.80","Medium",11207]
["8.81","Low",11208]
["8.82","Medium",11209]
["8.83","Low",11210]
["8.84","Low",11211]
["8.85","Medium",11212]
["8.86","Medium",11213]
["8.87","Medium",11214]
["8.88","Low",11215]
["8.89","High",11216]
["8.9","High",8577]
["8.90","High",11217]
["8.91","High",11218]
["8.92","Medium",11219]
["8.93","Low",11220]
["8.94","Low",11221]
["8.95","Medium",11222]
["8.96","Medium",11223]
["8.97","Low",11224]
["8.98","High",11225]
["8.99","Medium",11226]
["9.1","Low",8390]
["9.10","Medium",8399]
["9.11","Medium",8400]
["9.12","Medium",8401]
["9.13","Low",8402]
["9.14","Medium",8403]
["9.15","Medium",8404]
["9.16","High",8405]
["9.17","High",8406]
["9.18","Low",8407]
["9.19","Low",8408]
["9.2","Very High",8391]
["9.20","Medium",8409]
["9.21","Medium",8410]
["9.22","Low",8411]
["9.23","Low",8412]
["9.24","Medium",8413]
["9.25","Low",8414]
["9.26","Low",8415]
["9.27","Low",8416]
["9.28","Medium",8417]
["9.29","Low",8418]
["9.3","Very High",8392]
["9.4","High",8393]
["9.5","High",8394]
["9.6","Low",8395]
["9.7","Medium",8396]
["9.8","Medium",8397]
["9.9","Medium",8398]
["9.99","High",8419]

{"sheet":"Equipment_list","index":7,"n_rows":28,"n_cols":3,"rows_kept":28,"cut":false,"hidden":true,"merged":[]}
["TITLE","Equipment_list_description","ID"]
["Accommodation",null,12]
["Cargo Mach.",null,13]
["Critical Equip.",null,16]
["Deck - Machinery",null,18]
["Deck - Mooring Machinery",null,15]
["Deck - Pipe / Fittings",null,20]
["Documentation",null,21]
["E/R - Air Comp.",null,8]
["E/R - Aux. Engine",null,4]
["E/R - Aux. Mach.",null,7]
["E/R - Boiler",null,5]
["E/R - Main Engine",null,3]
["E/R - Pipes/ valves & fittings",null,9]
["E/R - Pumps",null,32]
["E/R - Purifier",null,6]
["Elect. Mach. & Equip.",null,10]
["Hull & Tanks",null,19]
["Inert Gas",null,14]
["LSA / FFA",null,17]
["Miscellaneous",null,22]
["Navigation - DGPS / EPFS / AIS",null,28]
["Navigation - ECDIS",null,25]
["Navigation - Echo Sounder / Speed Log",null,26]
["Navigation - GMDSS & Communication",null,23]
["Navigation - Others",null,11]
["Navigation - RADAR",null,24]
["Navigation - VDR / BNWAS",null,30]

{"sheet":"PSC_MOU","index":8,"n_rows":11,"n_cols":3,"rows_kept":11,"cut":false,"hidden":true,"merged":[]}
["TITLE","PSC_MOU_description","ID"]
["Asia and the Pacific",null,2]
["Caribbean",null,4]
["Europe and the North Atlantic",null,1]
["Latin America",null,3]
["The Black Sea region",null,6]
["The Indian Ocean",null,8]
["The Mediterranean",null,7]
["The Riyadh MoU",null,9]
["USCG",null,10]
["West and Central Africa",null,5]

{"sheet":"Inspection_type","index":9,"n_rows":13,"n_cols":2,"rows_kept":13,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Bunkering Audit",14]
["Cargo Audit",17]
["Engineering Audit",16]
["ISM Audit",2]
["ISPS Audit",3]
["IT Audit",10]
["MLC Audit",1]
["Mooring Audit",9]
["Nav Audit / Verification",8]
["Onboard Training",18]
["Ship Staff Insp.",15]
["Suptd. Insp.",13]

{"sheet":"Deficiency_Cause","index":10,"n_rows":8,"n_cols":3,"rows_kept":8,"cut":false,"hidden":true,"merged":[]}
["TITLE","Deficiency_Cause_description","ID"]
["Behaviour Based",null,1]
["Equipment Related",null,4]
["External Factors",null,5]
["Human Error",null,7]
["Inappropriate Procedure",null,8]
["Industry Issue",null,6]
["Knowledge Based",null,3]

{"sheet":"Observer_code","index":11,"n_rows":3,"n_cols":3,"rows_kept":3,"cut":false,"hidden":true,"merged":[]}
["TITLE","Observer_code_description","ID"]
["Owner / Marine / Tech. Suptd.",null,3]
["Ship Staff",null,2]

{"sheet":"Status_code","index":12,"n_rows":6,"n_cols":3,"rows_kept":6,"cut":false,"hidden":true,"merged":[]}
["TITLE","Status_code_description","ID"]
["Completed",null,6]
["Deferred to D D",null,5]
["In progress",null,3]
["Not Started",null,2]
["Waiting spare",null,4]

{"sheet":"PSC_ref_no","index":13,"n_rows":19,"n_cols":2,"rows_kept":19,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Alarms",9]
["Cargo operations including equipment",7]
["Certificates & Documentation",2]
["Dangerous Goods",13]
["Emergency Systems",5]
["Fire safety",8]
["ISM",16]
["ISPS",17]
["Life saving appliances",12]
["MLC, 2006",18]
["Other",19]
["Pollution Prevention",15]
["Propulsion and auxiliary machinery",14]
["Radio communication",6]
["Safety of Navigation",11]
["Structural condition",3]
["Water/Weathertight condition",4]
["Working and Living Conditions",10]

{"sheet":"Risk_value_of_obs","index":14,"n_rows":1,"n_cols":2,"rows_kept":1,"cut":false,"hidden":true,"merged":[]}
["Risk Value of observation","ID"]

{"sheet":"Year","index":15,"n_rows":18,"n_cols":1,"rows_kept":18,"cut":false,"hidden":true,"merged":[]}
["Year"]
[2014]
[2015]
[2016]
[2017]
[2018]
[2019]
[2020]
[2021]
[2022]
[2023]
[2024]
[2025]
[2026]
[2027]
[2028]
[2029]
[2030]

{"sheet":"Month","index":16,"n_rows":13,"n_cols":1,"rows_kept":13,"cut":false,"hidden":true,"merged":[]}
["Month"]
["Jan"]
["Feb"]
["Mar"]
["Apr"]
["May"]
["Jun"]
["Jul"]
["Aug"]
["Sep"]
["Oct"]
["Nov"]
["Dec"]

{"sheet":"Date_","index":17,"n_rows":32,"n_cols":1,"rows_kept":32,"cut":false,"hidden":true,"merged":[]}
["Date"]
["01"]
["02"]
["03"]
["04"]
["05"]
["06"]
["07"]
["08"]
["09"]
[10]
[11]
[12]
[13]
[14]
[15]
[16]
[17]
[18]
[19]
[20]
[21]
[22]
[23]
[24]
[25]
[26]
[27]
[28]
[29]
[30]
[31]

{"sheet":"Sheet1","index":18,"n_rows":24,"n_cols":6,"rows_kept":24,"cut":false,"hidden":true,"merged":[]}
[]
[null,"ID","E",null,"Date Recorded",1]
[null,"UNIQUE ID","F",null,"Type of Deficiency",2]
[1,"Date Recorded","G",null,"Observer code",3]
["ignore","Vessel Type","H",null,"Type of Inspection",4]
[null,"Internal / External","I",null,"Description of Deficiency",5]
[null,"Drydock","J",null,"Equipment Categories",6]
[null,"Information Sharing","K",null,"Area of Observation",7]
[null,"Critical_item","L",null,"Deficiency Cause",8]
[null,"Deficiency Type","M",null,"VIQ Ref Number",9]
[null,"Deficiency Cause","N",null,"Risk Value of Obs",10]
[null,"Inspection Type","O",null,"PSC Ref Number",11]
[null,"Equipments","P",null,"PSC MOU ID",12]
[null,"VIQ Reference Number","Q",null,"Action Taken or Required",13]
[null,"Risk Value of the observation","R",null,"Target Date",14]
[null,"PSC Reference Number","S",null,"PO Ref No.",15]
[null,"PSC MOU","T",null,"Status Code",16]
[null,"Observer Code","U",null,"Date Completed",17]
[null,"Target Date","V",null,"Drydock",18]
[null,"Status Code","W",null,"Info Sharing",19]
[null,"Description of Deficiency","X",null,"Critical Item Flag",20]
[null,"Action taken / required","Y",null,"Audit Type",21]
[null,"PO ref no","Z"]
[null,"Date completed","AA"]

{"sheet":"Ship_information","index":19,"n_rows":2,"n_cols":4,"rows_kept":2,"cut":false,"hidden":true,"merged":[]}
["Ship_ID","Ship_Name","FILE_NAME","Export_Date"]
["24","DHT BAUHINIA (22-07-2024)","24_1721633293627.xlsm","2024-08-06 02:08:91"]

{"sheet":"External_Deficiency_type","index":20,"n_rows":5,"n_cols":3,"rows_kept":5,"cut":false,"hidden":true,"merged":[]}
["TITLE","Type of deficiency_description","ID"]
["Condn of Class / Memo",null,5]
["Defect",null,1]
["Non Conformity",null,2]
["Observation",null,3]

{"sheet":"External_Inspection_type","index":21,"n_rows":11,"n_cols":2,"rows_kept":11,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Cargo Audit",17]
["Flag State Insp.",5]
["ISM Audit",2]
["ISPS Audit",3]
["MLC Audit",1]
["Nav Audit / Verification",8]
["OM Insp. (Eg. SIRE / CDI etc.)",6]
["Others (Eg. Insurance etc.)",12]
["PSC Inspection",4]
["Terminal Insp.",11]

{"sheet":"External_Observer_code","index":22,"n_rows":7,"n_cols":3,"rows_kept":7,"cut":false,"hidden":true,"merged":[]}
["TITLE","Observer_code_description","ID"]
["Class Surveyor",null,4]
["FSC Inspector",null,5]
["Others (Eg. Insurance etc.)",null,9]
["PSC Insp.",null,6]
["SIRE / CDI Insp.",null,8]
["Terminal Insp.",null,7]

{"sheet":"Sheet Version","index":23,"n_rows":2,"n_cols":2,"rows_kept":2,"cut":false,"hidden":true,"merged":[]}
["Version","Title"]
["2.0","Version 2.0"]