{"text_format":"1","workbook":"xlsx","n_sheets":24,"sheets":["Mainsheet","Completed","Calc","Areaofobs","Vessel_type","Deficiency_type","VIQrefno","Equipment_list","PSC_MOU","Inspection_type","Deficiency_Cause","Observer_code","Status_code","PSC_ref_no","Risk_value_of_obs","Year","Month","Date_","Sheet1","Ship_information","External_Deficiency_type","External_Inspection_type","External_Observer_code","Sheet Version"],"not_rendered":{"charts":0,"images":1,"macros":1,"external_links":0,"defined_names":12,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Mainsheet","index":0,"n_rows":31,"n_cols":28,"rows_kept":31,"cut":false,"hidden":false,"merged":[[10,8,10,9],[10,12,10,13],[12,6,12,27],[8,6,8,27]]}
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,"Defect - Damage Monitoring Sheet"]
[]
[null,null,null,null,null,null,null,"Date of Report","14-Oct-2024",null,null,"Ship Name","CAPE PHOENIX (11-08-2024)"]
[]
[null,null,null,null,null,null,"VERSION : 2.0"]
[]
[]
[]
[null,null,null,"ID","SHIPSIDE UNIQUEID","UNIQUE ID","Date Recorded","Type of Deficiency","Observer code","Type of Inspection","Description of Deficiency","Equipment Categories","Area of Observation","Deficiency Cause","VIQ Ref Number","Risk Value of Obs","PSC Ref Number","PSC MOU ID","Action Taken or Required","Target Date","PO Ref No.","Status Code","Date Completed","Drydock","Info Sharing","Critical Item","Audit Type","Superintendent Remarks"]
[null,null,null,null,93457,"129_Wed Jan 03 2024 17:33:30 GMT+0800","2024-03-29T08:00:00","Observation","Others (Eg. Insurance etc.)","Ship Staff Insp.","Water level guages of all ballast tanks are not operational.  water level guages in CCR  monitor displayed incorrect levels. with water level drop tank level does not drop and in some tanks, when in empty condition still display water levels. All guages to be calibrated or removed as it can lead to Rightship observation.","Hull & Tanks,Deck - Pipe / Fittings","Cargo / Ballast Systems","External Factors","","","","","Troubleshooting is carried out. Found system parameters faulty, same calibrated with externally connected transmitter. System side is working good condition. Found sensors defective. Requested to raise RO for spares from office.  Awaiting for owners advice.","2024-09-28T08:00:00","CPHO240146","Waiting spare",null,"No","No","No","Internal","Carry out troubleshooting as per autoelec dept and send the updates."]
[null,null,null,33059,12369,"129_Wed Nov 29 2023 11:22:01 GMT+0800","2024-04-28T23:59:35","Other","Ship Staff","Ship Staff Insp.","Fwd port and Starboard side Draft marks are faded and not readable below 13 meters","Hull & Tanks","Structural Condn. / WT integrity ","External Factors","","","","","Required Shore assistance to Paint the draft marks and can be done only in light ballast passage.","2024-09-28T23:59:35","","Not Started",null,"No","No","No","Internal","Liaise with agent and make arrangements to paint when vsl in berth."]
[null,null,null,null,97901,"129_Sat Jun 15 2024 16:52:31 GMT+0800","2024-06-02T08:00:00","Observation","Ship Staff","Ship Staff Insp.","Level gauge for waste oil tank is showing wrong reading.","Hull & Tanks","Eng. / Strg. Comp.","Equipment Related","","","","","Main wire and pointer wire replaced with new one.  Still operation found sluggish.\nSpring need to be renewed.  \nNew RO to be raised for the remaining necessary spares.\n\nWork in progress.","2024-07-29T08:00:00","Requisition CPHO240127 received.","In progress",null,"No","No","No","Internal","PO is under processing. Will be supplied in china."]
[null,null,null,null,40506,"129_Tue Aug 13 2024 08:29:36 GMT+0800","2024-08-12T08:00:00","Defect","Ship Staff","Ship Staff Insp.","REEFER CHAMBER OVERBOARD STORME VALVE SUSPECTED TO BE STUCKED AT CLOSED POSITION","E/R - Pipes/ valves & fittings","Structural Condn. / WT integrity ","Equipment Related","","","","","VALVE NEEDS TO BE REPLACED WITH NEW VALVE. DIVERS TO BE ARRANGED FOR BLANKING / PLUGGING FROM OVERBOARD. \n\n","2024-11-30T08:00:00","RO - CPHO240183 RECEIVED","Not Started",null,"No","No","No","Internal"]
[null,null,null,null,77465,"0_Thu Aug 15 2024 14:30:20 GMT+0800","2024-08-10T08:00:00","Defect","Ship Staff","Ship Staff Insp.","FIRE BILGE AND GS PUMP OVBD VALVE PH-004 STUCK IN 65% OPEN POSITION. ","E/R - Pipes/ valves & fittings","Structural Condn. / WT integrity ","Equipment Related","","","","","VALVE needs to be replaced. with diver assistance. Divers to be arranged for banking / plugging from overboard.\n","2024-12-10T08:00:00","Requisition CPHO240210 Received.","Not Started",null,"No","No","No","Internal"]
[null,null,null,null,12800,"129_Thu Aug 15 2024 15:52:16 GMT+0800","2024-08-15T08:00:00","Defect","Ship Staff","Ship Staff Insp.","NO.6 WBT VALVE NO: 011VPW & 012VPW IS NOT OPERATIONAL FROM REMOTE (BALLAST CONTROL CONSOLE) ","E/R - Pipes/ valves & fittings","Cargo / Ballast Systems","Equipment Related","","","","","011VPW AND 012VPW VALVE ACTUATOR FOUND NOT OPERATIONAL, ACTUATOR CONTROL PCB BOARD AND ELECTRIC MOTOR WAS HAVING MOISTURE, SAME REMOVED FROM POSITION AND CLEANED WITH ELECTRO SOLVE AND KEPT HALOGEN LIGHT FOR HEATING, ELECTRIC MOTOR OVERHAULED AND FOUND STATOR WINDINGS COMPLETELY SOAKED AND WAS BEYOND REPAIR, PRESENTLY THE VALVES ARE BEING OPERATED MANUALLY, NEED TO BE RENEWED WITH NEW ACTUATOR.\n\nRO CPHO240185 has been raised and awaiting for spares.","2024-11-15T08:00:00","RO -  CPHO240185 RAISED AND APPROVED.","Waiting spare",null,"No","No","No","Internal"]
[null,null,null,null,30395,"129_Thu Aug 15 2024 15:57:31 GMT+0800","2024-08-15T08:00:00","Defect","Ship Staff","Ship Staff Insp.","NO.6 WBT STRIPPING VALVE 014VPW IS NOT OPERATING FROM REMOTE (BALLAST CONTROL CONSOLE)","E/R - Pipes/ valves & fittings","Cargo / Ballast Systems","Equipment Related","","","","","014VPW STRIPPING VALVE ACTUATOR IS NOT OPERATIONAL, TROUBLESHOOTING CARRIED OUT AND FOUND ACTUATOR CONTROL PCB AND ELECTRICAL MOTOR WAS HAVING MOISTURE, CLEANING DONE USING ELECTRO SOLVE AND KEPT UNDER LIGHT FOR HEATING, HOWEVER THE PCB BOARD IS BEYOND REPAIR, PRESENTLY THE VALVE IS BEING OPERATED MANUALLY. \nRO CPHO240200 has been raised and awaiting for spares.","2024-11-15T08:00:00","RO CPHO240200 RAISED AND APPROVED.","Waiting spare",null,"No","No","No","Internal"]
[null,null,null,null,80162,"129_Fri Sep 13 2024 21:38:53 GMT+0800","2024-09-13T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Main engine jacket water cooler minor water leakage exists from the plate gasket.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Gasket to be replaced with new ones.  Spare ROB is 24 pcs. \nPlaning to replace all gaskets with new ones.\nNew RO - CPHO240245 raised for remaining spare gaskets.\nTo be replaced at an anchorage.  M/E immobilization permission required.","2024-10-31T08:00:00","Requisition  CPHO240209 received.\nNew RO - CPHO240245 raised and approved ","Not Started",null,"No","No","No","Internal"]
[null,null,null,null,46430,"129_Fri Sep 13 2024 21:41:36 GMT+0800","2024-09-13T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Main engine local console stop button 3 way valve found not functioning. ","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Vessel tried out the M/E local control from the engine side local controle console for both AHEAD and ASTERN direction several times and function found satisfactory. \nHowever the bell rings continuously throughout the testing period ( Local control ) untill change over back to the normal operation position.\n\nThe stop switch 3-way valve block found signs of an earlier open up for overhauling. No spare overhaul kit ROB. \nStop button pastic top was parted during testing and same repaired and placed back.\n\nThe 3-wat stop valve to be replaced with new spare.  one.\n========================================================================\nNew spare STOP button 3-way valve received and replaced with the faulty one on the M/E local control stand.\nThe M/E local control tried out and function found satisfactory.\nHowever the bell ( GONG )  continuously ringing without stopping since engaged the emergency operation rotary valve leaver to the emergency operation position, same as before.\nChecked the function of the limit switch of the conical clutch and found in order.\nTroubel shooting in progress.\n","2024-10-31T08:00:00","Requisition CPHO240192  Received","In progress",null,"No","No","No","Internal"]
[null,null,null,null,74215,"129_Sat Sep 14 2024 09:02:18 GMT+0800","2024-09-14T08:00:00","Defect","Ship Staff","Ship Staff Insp.","#1 HFO purifier found with a minor continuous oil leakage from the desludging port during opeartion.\nFound several places with pitting damage on the seating surface of the sliding bowl with the main sealing ring.","E/R - Purifier","Eng. / Strg. Comp.","Equipment Related","","","","","Purifire major overhaul carried out with following parts renewal.\nThe Vertical shaft renewed. New bearings assembled. All O-rings renewed, heavy liquid impeller, light liquid impeller, heavy liquid chamber, light liquid chamber, pilot valve and drain nozzle renewed. Clutch drum & pads renewed. \n539 – Lower Spring / 535 – Spring Seat / 536 – Steel Ball / 531 – Bearing Case / 533 – Spring Pin / 528 – Bearing Case / 537 – Bearing Cover / 510 – Bearing Case renewed. \nBoth oil inlet & outlet pressure sensor replaced with new spares.\nMulti monitor swap from the M/E lube oil purifier and put in to the HFO purifier and tried out. \nOperating water strainer before the regulating valve cleaned.\nOperating water time setting adjusted with continuous monitoring through sludge port.\nThe regulating valve for operating water supply renewed & Bowl closing timer increased.\nThe SV2 valve manually opened during the operation and found there is no any change in oil leakage.\nVessel tried out the M/E LO purifier complete bowl assembly on the #1 HFO \npurifier only for testing purpose about one and half day’s time and found operating without any oil leak from the desludging port during opeartion . All operational paramerers found normal. \nHowever with the original bowl assembly, a continuous oil leakage exists from the desludging port during opeartion. \n#1 HFO purifier bowl required reconditioning and balancing or complete bowl renewal.\nNew Sliding bowl received o/b and as instructed, the major parts of the bowl not recomended to change individually except complete renewal.\nAwaiting for office advice..","2024-10-13T08:00:00","Awaiting for advice from the office whether to recondition bowl or complete bowl renewal. Acordingly rais requisition.","Not Started",null,"No","No","No","Internal"]
[null,null,null,null,49512,"129_Sat Sep 14 2024 09:07:09 GMT+0800","2024-09-14T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Starboard side gangway motor gearbox oil found leaking. Part no 9 and part no 10 shafts found with heavy pitting. ","Deck - Machinery","Eng. / Strg. Comp.","Equipment Related","","","","","Shaft Seals renewed with matching seals. Need to carry out major overhauling with major parts renewal.\nvessel does not have spare shaft to replace. Also no other necessary spares available for the gangway gearboxes.\nGear box required complete overhauling with replacing new gear shafts as parts are badly pitted. \nThe PORT side gangway gear box also assumed to be in the same condition. Without necessary spares unable to open up and inspect. As preventive maintenance Both gear boxes required to be overhaulled.\nSTBD gearbox shaft cold work repaired by devcone and surface smoothen by an amery paper.\nGangway motor tried out and no leaks found. \nRO CPHO240227 has been raised and awaiting for spares.\n","2024-09-26T08:00:00","Requisition CPHO240227 raised and approved.","Waiting spare",null,"No","No","No","Internal"]
[null,null,null,null,93709,"129_Thu Oct 03 2024 08:13:48 GMT+0800","2024-10-01T08:00:00","Defect","Ship Staff","Ship Staff Insp.","CLutch facing of vaccum pump of both the Fire and GS pump and bilge & ballast pump found to be worn out.  It cannot engaged properly while pump at stop.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","","","","","Dismental the clutch and gave a try to adjust the spring.\nWhen spring adjust more, it makes more noice due to metal to metal contact of the clutch metal surfaces. Also noicy due to metal to metal slipping.\nSign of metal to metal contact is visible on the surface with scoring signs.\n\nThe clutch fiber surface clearly worn out and required to be renewed.\n\n","2024-11-30T08:00:00","RO CPHO 240234 raised and approved.","Waiting spare",null,"No","No","No","Internal"]
[null,null,null,null,14749,"129_Mon Oct 14 2024 16:50:04 GMT+0800","2024-10-07T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Bunker FOT 2(P) FWD steam coil indicated leaking coil as  the cascade tank water level reduces.","","Eng. / Strg. Comp.","Equipment Related","","","","","Bunker FOT 2(P) FWD steam coil isolated and blanked. \nFuel in the tank to be transfered to Bunker FOT 2(S)\nNew RO CPHO240249  raised fpr  INTERNAFTIKI METAL SUPER COATING. ","2024-12-31T08:00:00","RO CPHO240249 raised and approved","Waiting spare",null,"No","No","No","Internal"]
[null,null,null,null,85333,"129_Mon Oct 14 2024 16:55:16 GMT+0800","2024-10-05T08:00:00","Defect","Ship Staff","Ship Staff Insp.","#2 D/G tachometer showing an error of 50rpm as engine at stop condition and during the running condition, showing 950 rpm instead of 900 rpm.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Raised new RO - CPHO240246 for necessary tachometer","2024-11-30T08:00:00"," RO - CPHO240246 raised and approved","Waiting spare",null,"No","No","No","Internal"]

{"sheet":"Completed","index":1,"n_rows":172,"n_cols":28,"rows_kept":172,"cut":false,"hidden":false,"merged":[[10,8,10,9],[10,12,10,13],[12,6,12,27],[8,6,8,27]]}
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,"Defect - Damage Monitoring Sheet"]
[]
[null,null,null,null,null,null,null,"Date of Report","14-Oct-2024",null,null,"Ship Name","CAPE PHOENIX (11-08-2024)"]
[]
[null,null,null,null,null,null,"VERSION : 2.0"]
[]
[]
[]
[null,null,null,"ID","SHIPSIDE UNIQUEID","UNIQUE ID","Date Recorded","Type of Deficiency","Observer code","Type of Inspection","Description of Deficiency","Equipment Categories","Area of Observation","Deficiency Cause","VIQ Ref Number","Risk Value of Obs","PSC Ref Number","PSC MOU ID","Action Taken or Required","Target Date","PO Ref No.","Status Code","Date Completed","Drydock","Info Sharing","Critical Item","Audit Type","Superintendent Remarks"]
[null,null,null,24684,null,"129_23/3/2022 4:18:40 pm","2021-10-27T23:59:35","Defect","Ship Staff","Ship Staff Insp.","CONTROL AIR DRYER NOT WORKING\t","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","NEED TO BE REPLACE WITH NEW PART","2022-03-10T23:59:35","CPHO210028","Completed","2022-03-01T23:59:35","No","No","No","Internal"]
[null,null,null,24686,null,"129_23/3/2022 5:03:16 pm","2021-10-27T23:59:35","Observation","Ship Staff","Ship Staff Insp.","PRESS REGULATING VALVE NOT WORKING","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","F.O PRESSURE REGULATING VALVE REPLACED WITH NEW .","2022-03-10T23:59:35","CPHO210046","Completed","2022-04-10T23:59:35","No","No","No","Internal","to check spare received or not.  or cancelled your have to raise RO for 2022."]
[null,null,null,24687,null,"129_23/3/2022 5:41:42 pm","2021-10-27T23:59:35","Observation","Ship Staff","Ship Staff Insp.","AE 1&2 LO BACKWASH FILTER DIFF INDICATOR VALVES ARE LEAKING","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","valves renewed.","2022-03-10T23:59:35","CPHO210023","Completed","2022-03-08T23:59:35","No","No","No","Internal","to check spare received or not. or cancelled your have to raise RO for 2022."]
[null,null,null,24688,null,"129_23/3/2022 5:44:59 pm","2021-10-27T23:59:35","Observation","Ship Staff","Ship Staff Insp.","ME CYL LO FLOWMETER DAMAGED AT HINGED","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","flowmeter is made working.","2022-08-09T23:59:35","CPHO220125","Completed","2022-08-02T23:59:35","No","No","No","Internal","Spare ready on 8 July 2022.  will supply in next convenient port."]
[null,null,null,24689,null,"129_23/3/2022 5:47:35 pm","2021-10-27T23:59:35","Observation","Ship Staff","Ship Staff Insp.","BOILER FO PR SWITCH LEAKING FROM THE DIAPHARAM","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","pr.switch renewed with spare.","2022-03-10T23:59:35","CPHO210027","Completed","2022-03-03T23:59:35","No","No","No","Internal","spare should be delivered on board. please update"]
[null,null,null,24690,null,"129_2/4/2022 5:02:50 pm","2022-01-11T23:59:35","Observation","Ship Staff","Ship Staff Insp.","INCINERATOR SLUDGE PUMP LEAKING","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","leakage through seal arrested.","2022-04-10T23:59:35","","Completed","2022-03-21T23:59:35","No","No","No","Internal","to overhaul the pump, change the seal. if spare required please raise RO."]
[null,null,null,24691,null,"129_2/4/2022 5:06:55 pm","2022-01-12T23:59:35","Observation","Ship Staff","Ship Staff Insp.","BREAST FWD, SPRING FWD & AFT SPRING MOORING WINCH MOTOR BODY DAMAGED","Deck - Mooring Machinery","Eng. / Strg. Comp.","Equipment Related","","","","","Temporary repairs carried out as per Office Instructions , New Sapre Motor Received for Windlass and Mooring Winches- In Emergency same can be used upon Office approval- Defect Closed. ","2022-05-25T23:59:35","CPHO220015","Completed","2022-05-06T23:59:35","No","No","No","Internal","it has been repaired. to monitor the condition.  not require to change with new motor. spare will supply in next convenient port.  to close the defect if spare motor receive"]
[null,null,null,24693,null,"129_2/4/2022 4:56:55 pm","2022-03-06T23:59:35","Observation","Ship Staff","Suptd. Insp.","AE FO LINE PR REGULATING VALVE MALFUNCTIONING","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Valve is operating satisfactorily","2022-10-11T23:59:35","CPHO220107 RAISED FOR SERVICE KIT.","Completed","2022-08-13T23:59:35","No","No","No","Internal","to overhaul the valve first,  RO for spare waiting readiness will supply next convenient port"]
[null,null,null,24952,37025,"129_Tue Apr 19 2022 15:22:46 GMT+0800","2022-03-17T23:59:35","Observation","Ship Staff","Ship Staff Insp.","ALL ROLLER FAIRLEAD- TO DISMANTLE AND DERUST","Deck - Mooring Machinery","Mooring","Equipment Related","","","","","All 58 fairlead rollers removed from shaft, hydroblasted, cleaned, derusted and painted. Derusting and painting of shaft and base carried out. Greasing carried out. Grease nipple inspected, cleaned and mounted back. All rollers mounted back in position with covers. All fairlead rollers now in good working condition.\nFinal Cosmetic painting and marking in progress.","2022-06-16T23:59:35","","Completed","2022-05-10T23:59:35","No","No","No","Internal","to carry out and complete before target date"]
[null,null,null,25230,57571,"129_Fri Apr 29 2022 01:34:17 GMT+0800","2022-03-17T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","AREAS IN ENGINE CASING TO CLEAN AND PAINT, CHECK ALL LIGHTS.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","CLEANING AND PAINTING  OF ENGINE ROOM CASING AREA CARRIED OUT AND ALL BUSTED LAMPS RENEWED.","2022-05-17T23:59:35","","Completed","2022-04-16T23:59:35","No","No","No","Internal","to carry out and complete before target date"]
[null,null,null,25232,95662,"129_Fri Apr 29 2022 01:25:43 GMT+0800","2022-03-17T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","\tSHIP SIDE\tSHIP SIDE STRUCTURE NEAR MAIN ENGINE L.O AUTOBACKWASH FILTER TO DERUST AND PAINT\t\t\t","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","SHIP SIDE DERUSTED AND APPLIED WHITE PAINT.","2022-04-16T23:59:35","","Completed","2022-03-30T23:59:35","No","No","No","Internal"]
[null,null,null,25233,41057,"129_Fri Apr 29 2022 01:28:16 GMT+0800","2022-03-17T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","CENTRAL COOLER SW INLET PIPE LEAKAGE TO RECTIFY.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","PIPE REPLACED WITH SPARE SACRIFICIAL PIPE.","2022-04-06T23:59:35","","Completed","2022-04-07T23:59:35","No","No","No","Internal"]
[null,null,null,25234,77543,"129_Fri Apr 29 2022 01:30:55 GMT+0800","2022-03-17T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","FRESH HYD TANK DISCHARGE VALVE LEAKING CAUSE PUMP REVERSE ROTATION WHEN STOP PERIODE","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","VALVE REPLACED WITH OVERHAULED ONE , PUMP DOES NOT ROTATE ON STOP CONDITION.","2022-04-01T23:59:35","","Completed","2022-03-30T23:59:35","No","No","No","Internal"]
[null,null,null,25235,34832,"129_Fri Apr 29 2022 01:36:33 GMT+0800","2022-03-17T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","FWG CONDENSOR S.W PIPE LEAK TO RECTIFY AND PAINT THE NEW FABRICATED PIPE.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","NEW PIPE FABRICATED ,FITTED AND PAINT APPLIED.","2022-04-01T23:59:35","","Completed","2022-03-21T23:59:35","No","No","No","Internal"]
[null,null,null,25236,95792,"129_Fri Apr 29 2022 01:39:03 GMT+0800","2022-03-17T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","A/E JACKET COOLER SAVE ALL TO CLEAN AND PAINT","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","SAVE ALL CHIPPED AND DERUSTED , PAINTING CARRIED OUT.","2022-04-06T23:59:35","","Completed","2022-04-04T23:59:35","No","No","No","Internal"]
[null,null,null,25222,81387,"129_Wed Apr 27 2022 00:28:42 GMT+0800","2022-03-18T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","HATCH COVER HEAVY BOLT TO CARRY OUT MAINTENANCE","Cargo Mach.","Structural Condn. / WT integrity ","Equipment Related","","","","","DERUSTING AND LUBRICATION","2022-05-17T23:59:35","","Completed","2022-04-25T23:59:35","No","No","No","Internal","to carry out as per plan and keep update"]
[null,null,null,25223,92969,"129_Wed Apr 27 2022 00:31:17 GMT+0800","2022-03-18T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","HATCH COVER GAS SAMPLING POINT FROZEN IN SOME PLACES","Cargo Mach.","Structural Condn. / WT integrity ","Equipment Related","","","","","TO DERUST AND LUBRICATE THREAD/ Threads are worn out and beyond repair, De-rusting and Lubrication done and completed;// spares-CPHO220140 received and job in progress, Job completed on 24th June 2022. DEFECT CLOSED.","2022-06-17T23:59:35","CPHO220140","Completed","2022-06-03T23:59:35","No","No","No","Internal","RO has been supplied.  job to be carry out as necessary. only damaged one required to change."]
[null,null,null,25224,64325,"129_Wed Apr 27 2022 00:36:07 GMT+0800","2022-03-18T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","HATCH COVER CENTER STOPPER-MAINTENANCE","Cargo Mach.","Structural Condn. / WT integrity ","Equipment Related","","","","","TO DE RUST, CHECK AND PAINT// JOB COMPLETED- DEFECT CLOSED","2022-06-16T23:59:35","","Completed","2022-06-15T23:59:35","No","No","No","Internal","to carry out and complete before target date"]
[null,null,null,25225,69172,"129_Wed Apr 27 2022 00:33:12 GMT+0800","2022-03-18T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","STBD SIDE ENTRANCE PLATFORM STEP- OBSERVED TO BE WEAK","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","Equipment Related","","","","","Reinforced the Step by additional Bracket installed","2022-05-17T23:59:35","","Completed","2022-05-09T23:59:35","No","No","No","Internal","to carry out and complete asap"]
[null,null,null,25226,12193,"129_Wed Apr 27 2022 00:38:12 GMT+0800","2022-03-20T23:59:35","Non Conformity","Ship Staff","Ship Staff Insp.","RESCUE BOAT DECK SAFETY RAILINGS- FOR ADDITIONAL 1 DETTACHABLE RAILING","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","TO RAISE RO AND INSTALL // New Chain installed - Defect Closed","2022-06-19T23:59:35","CPHO220110","Completed","2022-05-10T23:59:35","No","No","No","Internal","to raise Ro as required, will supply at next convenient port"]
[null,null,null,25227,72222,"129_Wed Apr 27 2022 00:42:18 GMT+0800","2022-03-20T23:59:35","Observation","Ship Staff","Ship Staff Insp.","MF/HF ANTENNA- DETERIORATED SAFETY CHAIN GUARD","Navigation - GMDSS & Communication","Structural Condn. / WT integrity ","External Factors","","","","","TO RENEW// Renewed all 3 Chains with New SS chains- Defect closed","2022-06-19T23:59:35","CPHO220110","Completed","2022-05-10T23:59:35","No","No","No","Internal","RO will supply next convenient port"]
[null,null,null,25228,74485,"129_Wed Apr 27 2022 00:44:15 GMT+0800","2022-03-20T23:59:35","Observation","Ship Staff","Ship Staff Insp.","GANGWAY UPPER PLATFORM-SUBJECT FOR THOROUGH INSPECTION","Deck - Machinery","Structural Condn. / WT integrity ","Equipment Related","","","","","TO DISMANTLE, DERUST AND INSPECT// STBD Gangway maintenance completed in May 20th 2022 // completed inspection and maintenance of Port Accommodation ladder on 07th July 2022.","2022-06-19T23:59:35","CPHO220141","Completed","2022-06-16T23:59:35","No","No","No","Internal","spare has been confirmed and  will supply next convenient port."]
[null,null,null,25231,82551,"129_Fri Apr 29 2022 01:21:02 GMT+0800","2022-03-21T23:59:35","Observation","Ship Staff","Ship Staff Insp.","BALLAST PUMP #2 WORKING STAND CORRODED ,HOLED.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","NEW PLATE FOR STAND TO FABRICATE AND FIX.","2022-04-09T23:59:35","","Completed","2022-03-25T23:59:35","No","No","No","Internal"]
[null,null,null,25237,25102,"129_Fri Apr 29 2022 01:41:44 GMT+0800","2022-03-21T23:59:35","Defect","Ship Staff","Ship Staff Insp.","AUX.ENGINE L.T COOLER S.W INLET PIPE LEAKING.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","LEAKING PIPE REPLACED WITH NEW ONE.","2022-04-09T23:59:35","","Completed","2022-04-06T23:59:35","No","No","No","Internal"]
[null,null,null,25238,53563,"129_Fri Apr 29 2022 01:44:16 GMT+0800","2022-03-22T23:59:35","Defect","Ship Staff","Ship Staff Insp.","MAIN ENGINE L.O COOLER S.W INLET PIPE HAVE SOFT PATCH/ LEAKING.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","SYSTEM ISOLATED AT ANCHORAGE , PIPE REMOVED AND WELD REPAIRS CARRIED OUT IN WORKSHOP AND FITTED BACK./ JOB COMPLETED AT SALDANHA BAY ANCHORAGE.","2022-04-09T23:59:35","","Completed","2022-04-07T23:59:35","No","No","No","Internal"]
[null,null,null,25288,14754,"129_Sat May 07 2022 17:32:15 GMT+0800","2022-04-13T23:59:35","Defect,Observation","Ship Staff","Ship Staff Insp.","AUX.ENGINE #1 AIR COOLER COOLING WATER OUTLET PIPE LEAKING.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","PIPE LINE REMOVED 0 RINGS RENEWED AND LEAK RECTIFIED.","2022-05-19T23:59:35","","Completed","2022-04-18T23:59:35","No","No","No","Internal","if the job complete your can insert the completion date to close the defect"]
[null,null,null,25229,71821,"129_Wed Apr 27 2022 00:45:35 GMT+0800","2022-04-19T23:59:35","Observation","Ship Staff","Ship Staff Insp.","HATCH COVER VENT AND HOLD ACCESS RUBBER PACKING","Cargo Mach.","Structural Condn. / WT integrity ","Equipment Related","","","","","SUBJECT FOR REPLACEMENT// HATCH COVER VENT AND HOLD ACCESS RUBBER PACKING RENEWED_ DEFECT CLOSED","2022-07-20T23:59:35","CPHO220110","Completed","2022-07-22T23:59:35","No","No","No","Internal","RO has been supplied on board. please carry out as required"]
[null,null,null,25467,71509,"129_Thu May 19 2022 10:50:29 GMT+0800","2022-04-25T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Deck Main Fire Line and branch fire line in deteriorated condition and leaking","Deck - Pipe / Fittings,LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","Through inspection of the entire Fire line carried out, found Four Nos of leaking areas in the Main fire line and Soft patches at various Locations, Need renewal of Fire Line approx. 160 Mtrs in Length including Branch fire line and Dresser Couplings, 9 Sections of 6 Mts main fire line Renewal completed on 29th May 2022.// Branch fire line 65A completed on 5th June 2022// Painting and derusting of Branch fire line 65A in progress will be completed on 21st June 2022.// Fire line renewal Job completed on 07th July 2022- Defect CLOSED.","2022-07-01T23:59:35","CPHO220142","Completed","2022-06-16T23:59:35","No","No","No","Internal","to update office status till the job complete"]
[null,null,null,25468,91202,"129_Mon May 30 2022 09:46:11 GMT+0800","2022-04-29T23:59:35","Defect","Ship Staff","Ship Staff Insp.","WBT - TST -2 STBD, Transverse Frame NO 259 found dent and deformed about 60 cm , TST frame deformed area is just above the summer Load line and the area found heavily rusted, No any cracks found on the Frame and the adjacent frames","Hull & Tanks","Structural Condn. / WT integrity ","External Factors","","","","","Through inspection to be done by Class NKK and appropriate action to be taken during the next DD as per Class advise// Ship staff de-rusted the rusted area and applied 2 coat of paint.//  job to shifted to DD spec. closed the job for DDRL ","2024-01-09T23:59:35","","Completed","2022-05-17T23:59:35","No","No","No","Internal","Noted. job to shift to DD spec. close the job for DDRL once painting job complete"]
[null,null,null,25469,30434,"129_Mon May 30 2022 14:03:03 GMT+0800","2022-04-29T23:59:35","Defect","Ship Staff","Ship Staff Insp.","operating water solenoid assembly for main  L.O purifier ,manual opertion switch is broken and hence valve is stuck in open position  making the l.o purifier non operational.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","spares received and solenoid valve assembly fitted , purifier tried out satisfactory.","2022-08-09T23:59:35","CPHO220147 raised.","Completed","2022-08-02T23:59:35","No","No","No","Internal","Spare confirmed and waiting for readiness. will supply once collect."]
[null,null,null,25470,83534,"129_Mon May 30 2022 14:05:46 GMT+0800","2022-05-04T23:59:35","Observation","Ship Staff","Ship Staff Insp.","galley air con cooling sea water inlet pipe is corroded and leaking.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","condensor end cover threads coroded hence pipe is welded with end cover and leak rectified.","2022-08-04T23:59:35","","Completed","2022-05-24T23:59:35","No","No","No","Internal","to complete before due date"]
[null,null,null,25629,47334,"129_Sun Jun 12 2022 14:41:12 GMT+0800","2022-05-12T23:59:35","Observation","Ship Staff","Ship Staff Insp.","steam leak from flange of the excess steam control valve.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","main steam stop valve to shut, steam to isolate & leak to rectify.\nsteam isolated and leak rectified.","2022-05-25T23:59:35","","Completed","2022-05-22T23:59:35","No","No","No","Internal"]
[null,null,null,25923,38456,"129_Sat Jun 25 2022 10:03:23 GMT+0800","2022-05-31T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Erratic readings -midship port and stbd draft level gauges","Hull & Tanks","Cargo / Ballast Systems","Equipment Related","","","","","•\tOn dismantling the sensors it is observed that the electric terminals are grounded and the sensor was filled up with hard deposits of salt indicating sea water passing through the seals to the electric terminals.\n•\tPort side sensor was observed damaged with hard deposits on electrical terminals , same after cleaning the resistance value was found to be 4 Mohms\n•\tStbd  sensor cleaned up the deposits and sealing rings were renewed from 0 ring kit, resistance check carried out and found value to be 15 Mohms.\n•        As per the checks suspecting the sensors are defective and need replacement.\n\n•        Have raised requisition (CPHO220156: pressure electric type draft sensor) for the sensors\n spares received on 14/07/2022, job  will complete job by 20th July 2022// Flag dispensation taken on 24th June 2022 till 30th Sep 2022// New sensors install, all working in good order. Defect closed on 20th July 2022.","2022-09-09T23:59:35","CPHO220156","Completed","2022-06-29T23:59:35","No","No","No","Internal","spare already on board. please carry out and update"]
[null,null,null,26156,25376,"129_Wed Jul 13 2022 14:20:45 GMT+0800","2022-06-11T23:59:35","Observation","Ship Staff","Ship Staff Insp.","main engine l.o cooler s.w outlet pipe line is corroded and holed.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","s.w leak is arrested with help of clamp, pipe line to renew at next port./\npipe line replaced with new one .","2022-06-25T23:59:35","","Completed","2022-06-23T23:59:35","No","No","No","Internal"]
[null,null,null,27607,22122,"129_Tue Oct 04 2022 17:36:14 GMT+0800","2022-09-15T23:59:35","Observation","Ship Staff","Ship Staff Insp.","#4 MOORING WINCH LEAKING OIL FROM REDUCTION GEAR SIDE.","Deck - Mooring Machinery","Mooring","Equipment Related","","","","","OIL SEAL FOUND TO BE DAMAGED. SAME RENEWED",null,"CPHO220224","Completed","2022-11-18T23:59:35","No","No","No","Internal","Spare could be supplied to vessel. to updated status"]
[null,null,null,24685,null,"129_23/3/2022 4:14:33 pm","2022-09-26T23:59:35","Observation","Ship Staff","Ship Staff Insp.","STEERING GEAR 1&2 LEAKING FROM SERVO CONTROLLER UNITS AND RAMS","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Ram leakages rectefied. No.1 S/G servo motor leak rectefied.","2023-02-12T23:59:35","CPHO 220020","Completed","2023-02-02T23:59:35","No","No","No","Internal","spare already on board. to rectify at the first opportunity. this job to carry out by ship staff."]
[null,null,null,24692,null,"129_2/4/2022 4:53:10 pm","2022-09-26T23:59:35","Observation","Ship Staff","Ship Staff Insp.","LS FO SETT TANK LEVEL GAUGE DAMAGED","Hull & Tanks","Eng. / Strg. Comp.","Equipment Related","","","","","Job completed gauge is working in order.","2023-02-12T23:59:35","CPHO220094","Completed","2023-02-01T23:59:35","No","No","No","Internal","spare confirmed and will supply in next convenient port"]
[null,null,null,29803,19464,"129_Tue Mar 21 2023 09:26:08 GMT+0800","2023-01-09T23:59:35","Non Conformity","Ship Staff","Ship Staff Insp.","Lifebuoys are painted  which is a fire hazard and Prevent any damages/crack to the buoys on Inspection. ","LSA / FFA","Safety / LSA / FFA","Human Error","","","","","Lifebuoys received in Bayuquan China and all lifebuoys replaced which were painted including MOB lifebuoys of 4.5 Kgs.","2023-01-23T23:59:35","","Completed","2023-01-27T23:59:35","No","No","No","Internal"]
[null,null,null,29810,66931,"129_Wed Mar 29 2023 00:31:45 GMT+0800","2023-01-09T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Main Deck Abreast Port side HC No.1 rusted 35-40%. Require derusting and painting.","","General Appearance","External Factors","","","","","Completed derusting and painting main deck port side abreast No.1 HC. Now in good condition.","2023-03-15T23:59:35","","Completed","2023-03-02T23:59:35","No","No","No","Internal"]
[null,null,null,29804,51214,"129_Tue Mar 21 2023 09:29:22 GMT+0800","2023-01-15T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Port and stbd pilot access ladder's Nut and bolt which is joining the Upper platform and the ladder is thinned down and wasted.","Deck - Machinery","Safety / LSA / FFA","Equipment Related","","","","","Renewed the Nut and bolt for both the Pilot Access Ladder.","2023-02-20T23:59:35","","Completed","2023-03-04T23:59:35","No","No","No","Internal"]
[null,null,null,29811,13692,"129_Wed Mar 29 2023 00:38:11 GMT+0800","2023-01-15T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Hatch cover quick actings cleats are rusted and require derusting.  Cleats are also found in frozen condition.","Hull & Tanks","Structural Condn. / WT integrity ","External Factors","","","","","Completed All hatch cover quick acting cleats dismantling, freeing and Derusting/painting. Now in Good condition.","2023-03-15T23:59:35","","Completed","2023-03-12T23:59:35","No","No","No","Internal"]
[null,null,null,29801,66009,"129_Sun Feb 26 2023 18:45:12 GMT+0800","2023-01-17T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Catwalk grating between HC No.1 and 2 found wasted.","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","External Factors","","","","","Renewed Gratings and frame of Catwalk between HC No.1 and 2.","2023-02-12T23:59:35","","Completed","2023-02-07T23:59:35","No","No","No","Internal"]
[null,null,null,29813,70665,"129_Wed Mar 29 2023 12:36:43 GMT+0800","2023-01-17T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Inclinometer found fabricated onboard and presently angle indicator frozen on Port and stbd gangway. ","Deck - Pipe / Fittings","Safety / LSA / FFA","Human Error,Inappropriate Procedure,Knowledge Based","","","","","Renewed Inclinometer for port and stbd gangway.","2023-02-12T23:59:35","","Completed","2023-02-20T23:59:35","No","No","No","Internal"]
[null,null,null,29814,50517,"129_Wed Mar 29 2023 12:38:59 GMT+0800","2023-01-17T23:59:35","Non Conformity","Ship Staff","Ship Staff Insp.","Inclinometer found missing from Port and stbd Pilot access ladders.","Deck - Pipe / Fittings","Safety / LSA / FFA","External Factors,Human Error,Inappropriate Procedure,Knowledge Based","","","","","Frame fabricated and New angle inclinometer installed on Port and stbd Pilot access ladder.","2023-02-12T23:59:35","","Completed","2023-01-23T23:59:35","No","No","No","Internal"]
[null,null,null,29800,94253,"129_Fri Feb 17 2023 04:51:31 GMT+0800","2023-01-21T23:59:35","Non Conformity","Ship Staff","Ship Staff Insp.","Carried out light /chalk test of weathertight doors, A deck Port side upper and A deck, stbd side A deck and Aft provision store weathertight door failed Test. Retaining channel rubber to renew and dogged handle to be dismantle and repair for proper closure","Accommodation","Structural Condn. / WT integrity ","Knowledge Based","","","","","Retaining channel derusted and painted. Rubber packing renewed of all leaking doors. Dogged handles dismantled and greased and fitted back.","2023-02-04T23:59:35","","Completed","2023-01-25T23:59:35","No","No","No","Internal"]
[null,null,null,29816,84459,"129_Tue Mar 21 2023 09:44:50 GMT+0800","2023-01-22T23:59:35","Defect","Ship Staff","Ship Staff Insp.","VALVE 001VPW IS NOT OPERABLE FROM SHIP'S OFFICE CONSOLE AND REQUIRED TO BE OPEN MANUALLY FROM ENGINE ROOM","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","Defect rectefied.Valve operation checked from console.Working in order.","2023-03-14T23:59:35","","Completed","2023-03-05T23:59:35","No","No","No","Internal"]
[null,null,null,29812,96649,"129_Wed Mar 29 2023 11:56:32 GMT+0800","2023-01-23T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Securing arrangement for chains on main deck have thinned down and some have been wasted. ","Deck - Pipe / Fittings","Safety / LSA / FFA","Inappropriate Procedure,Human Error","","","","","All Securing arrangement of chains inspected and whichever were thinned down or wasted renewed.","2023-03-15T23:59:35","","Completed","2023-03-11T23:59:35","No","No","No","Internal"]
[null,null,null,29806,25285,"129_Tue Mar 21 2023 09:41:33 GMT+0800","2023-01-24T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Catwalk grating between HC No.3 and 4 found wasted.","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","Industry Issue","","","","","RENEWED FRAME AND GRATINGS ON CROSS DECK BETWEEN HC No.3 AND 4.","2023-03-15T23:59:35","","Completed","2023-03-05T23:59:35","No","No","No","Internal"]
[null,null,null,29805,21195,"129_Tue Mar 21 2023 09:35:21 GMT+0800","2023-01-31T23:59:35","Defect","Ship Staff","Ship Staff Insp.","GANGWAY PORT AND STBD ROLLER FOUND DAMAGED. ","Hull & Tanks","Structural Condn. / WT integrity ","Knowledge Based","","","","","BOTH PORT AND STBD GANGWAY ROLLERS RENEWED.","2023-03-09T23:59:35","","Completed","2023-03-05T23:59:35","No","No","No","Internal"]
[null,null,null,29802,61570,"129_Mon Feb 27 2023 08:49:33 GMT+0800","2023-02-11T23:59:35","Defect","Ship Staff","Ship Staff Insp.","SW cooling discharge pipe ruptured due to material failure","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Defective pipe removed repairs carried out and fitted back, tested and found in order.New pipe fabrication completed and kept as spare.","2023-03-11T23:59:35","","Completed","2023-02-19T23:59:35","No","No","No","Internal"]
[null,null,null,29789,29931,"129_Thu Mar 30 2023 10:57:08 GMT+0800","2023-02-12T23:59:35","Defect,Observation","Ship Staff","Ship Staff Insp.","All goose neck ventilators on accommodation block require derusting and painting.","Accommodation","General Appearance","Human Error,External Factors,Industry Issue","","","","","completed derusting and painting of all Goose neck ventilators on accommodation blocks.","2023-05-15T23:59:35","","Completed","2023-04-27T23:59:35","No","No","No","Internal","please keep update."]
[null,null,null,29796,21706,"129_Wed Mar 29 2023 15:52:40 GMT+0800","2023-02-20T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Main deck Port side Abreast HC No.2, main deck abreast cross deck HC No.1&2 and 2&3 is rusted and require derusting and painting.","Hull & Tanks","General Appearance","External Factors","","","","","Completed derusting and painting.","2023-04-29T23:59:35","","Completed","2023-04-04T23:59:35","No","No","No","Internal","please keep update."]
[null,null,null,29795,29700,"129_Wed Mar 29 2023 15:50:56 GMT+0800","2023-02-21T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Cross Deck btw HC 2 and 3 require extensive derusting and painting. Derusting of Booby hatches and manholes cover also to be carried out on Cross deck btw #2 and 3.","Hull & Tanks","General Appearance","External Factors","","","","","Completed derusting and painting.","2023-04-29T23:59:35","","Completed","2023-04-01T23:59:35","No","No","No","Internal","Please expedite."]
[null,null,null,29988,24328,"129_Sat May 13 2023 13:36:32 GMT+0800","2023-02-28T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Cross deck 3 and 4 heavily rusted, require derusting and painting.","Hull & Tanks","General Appearance","External Factors","","","","","Completed derusting and painting.","2023-04-30T23:59:35","","Completed","2023-03-28T23:59:35","No","No","No","Internal"]
[null,null,null,29808,77807,"129_Fri Mar 24 2023 11:18:57 GMT+0800","2023-03-05T23:59:35","Observation","Ship Staff","Ship Staff Insp.","# 6 mooring winch reduction gear side seal to be renewed","Deck - Mooring Machinery","","Equipment Related","","","","","Seal renewed and system tried out.Operation in order","2023-03-15T23:59:35","","Completed","2023-03-08T23:59:35","No","No","No","Internal"]
[null,null,null,29809,51061,"129_Fri Mar 24 2023 12:25:21 GMT+0800","2023-03-05T23:59:35","Observation","Ship Staff","Ship Staff Insp.","# 8 Mooring winch reduction gear side seal to renew","Deck - Mooring Machinery","","Equipment Related","","","","","reduction gear side seal renewed. System tried out. Operation in order.","2023-03-15T23:59:35","","Completed","2023-03-12T23:59:35","No","No","No","Internal"]
[null,null,null,29807,90587,"129_Wed Mar 22 2023 02:28:30 GMT+0800","2023-03-06T23:59:35","Observation","Ship Staff","Ship Staff Insp.","#7 MOORING WINCH REDUCTION GEAR SIDE SEAL TO RENEW ","Deck - Mooring Machinery","Mooring","Equipment Related","","","","","seal renewed and system tried out.Operation found in order.","2023-03-15T23:59:35","","Completed","2023-03-07T23:59:35","No","No","No","Internal"]
[null,null,null,29986,69790,"129_Sat May 13 2023 13:41:49 GMT+0800","2023-03-07T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Cross deck Btw 4&5, 5&6 and 6&7 require derusting and painting. Excessive rust visible","Hull & Tanks","General Appearance","External Factors","","","","","Derusting & painting top coat completed on cross deck Btw 4&5 and 6&7 & 5&6 #.","2023-05-31T23:59:35","","Completed","2023-05-17T23:59:35","No","No","No","Internal"]
[null,null,null,29792,11234,"129_Tue Mar 21 2023 09:39:07 GMT+0800","2023-03-15T23:59:35","Defect","Ship Staff","Ship Staff Insp.","RUBBER WASHERS OF QUICK ACTING CLEATS OF HATCH COVERS ARE IN POOR CONDITION AND HAVE LOST ELASTICITY. REQUIRE TO BE RENEWED.","Hull & Tanks","Structural Condn. / WT integrity ","Inappropriate Procedure","","","",""," Renewal of rubber washers of cleats has been done.","2023-08-17T23:59:35","","Completed","2023-08-15T23:59:35","No","No","No","Internal",""]
[null,null,null,29790,68910,"129_Tue Mar 21 2023 09:23:06 GMT+0800","2023-03-16T23:59:35","Non Conformity","Ship Staff","Ship Staff Insp.","Fireman outfits are in very poor condition. pants and jackets are torn. helmet not covering entire neck.","LSA / FFA","Safety / LSA / FFA","Industry Issue","","","","","REQN No-CPHO230044, received on 10 July at Singapore. Fireman outfits which are in very poor condition renewed. New helmet received covering entire neck and renewed.","2023-07-16T23:59:35","","Completed","2023-06-26T23:59:35","No","No","No","Internal","will supply at next convenient port."]
[null,null,null,29989,25132,"129_Sat May 13 2023 13:39:08 GMT+0800","2023-03-17T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Port side main deck abreast hatch cover 3  requires derusting. % of rust is more than 30%","Hull & Tanks","General Appearance","External Factors","","","","","Completed derusting and painting","2023-04-30T23:59:35","","Completed","2023-04-05T23:59:35","No","No","No","Internal"]
[null,null,null,29815,58007,"129_Wed Apr 12 2023 14:02:33 GMT+0800","2023-03-22T23:59:35","Observation","Ship Staff","Ship Staff Insp.","# 1 Mooring winch reduction gear side seal to renew","Deck - Mooring Machinery","","Equipment Related","","","","","reduction gear side seal renewed. System tried out. Operation found in order.","2023-04-14T23:59:35","","Completed","2023-03-27T23:59:35","No","No","No","Internal"]
[null,null,null,29798,83536,"129_Wed Apr 05 2023 23:15:57 GMT+0800","2023-03-24T23:59:35","Defect","Ship Staff","Nav Audit / Verification","ECDIS JRC-901B - 1 set zoom out button is defective. If pressed once, continuous zooming in Occurs. Require to renew the button. No damages to the button.","Navigation - ECDIS","Navigation","Equipment Related","","","","","Rectified action has been done properly by shore service provider . ECDIS JRC-901B - 1 set zoom out button is working functionally.  ","2023-06-16T23:59:35","","Completed","2023-06-15T23:59:35","No","No","No","Internal","please send separate email to AUTOELEC SUPPORT for follow up."]
[null,null,null,29984,52015,"129_Tue May 09 2023 17:07:03 GMT+0800","2023-04-16T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Control air dryer disposable membrane filter is out of operation as it is clogged. Vessel does not have spare on board. ","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Vessel received spare and installed the new control air dryer and put in use, working satisfactory.","2023-06-15T23:59:35","CPHO230082","Completed","2023-06-20T23:59:35","No","No","No","Internal"]
[null,null,null,29990,91785,"129_Sat May 13 2023 13:45:38 GMT+0800","2023-04-16T23:59:35","Non Conformity","Ship Staff","Ship Staff Insp.","Center Cleats of all hatch covers to be freed and rubber washer to be replaced.","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","External Factors","","","","","Rubber washer of all Hatch cover From No 2 to 9 renewed. Center cleats freed and greased.  Now in battened down position. ","2023-05-15T23:59:35","","Completed","2023-04-28T23:59:35","No","No","No","Internal"]
[null,null,null,29983,11329,"129_Tue May 09 2023 16:56:30 GMT+0800","2023-05-16T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Suction pipeline from sea chest to Ref. Machinery C.S.W pump has found with patches with minor leakage.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","During anchorage Brazil, Itaguai, cooling of A/E was done by external seawater firehose , connected to LT cooler from Emergency fire pump. All sea chest was closed and drained the water. Pipe was removed and modified new one. Water opened, tested , all found ok, not any leakage anymore .Not any remarks. Photos with job done was sent by \" Daily work done by Engine\" . ","2023-08-15T23:59:35","","Completed","2023-08-07T23:59:35","No","No","No","Internal"]
[null,null,null,29987,89061,"129_Tue May 09 2023 16:48:06 GMT+0800","2023-05-16T23:59:35","Defect","Ship Staff","Ship Staff Insp.","C.S.W pump discharge pipeline to AE LT cooler found patches with minor leakages. ","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","During anchorage Brazil / Itaguai, cooling of AE's was done by external sea water fire hose, connected to LT cooler, from Em-cy Fire Pump. All sea chest was closed, and drain the water. Pipe was removed out, and fabricate new one. Water opened, tested, all found ok, not any leakage anymore. Not any remarks. Photos with job done was sent by \" Daily work done by Engine\", to the Office.\n","2023-08-15T23:59:35","","Completed","2023-08-06T23:59:35","No","No","No","Internal"]
[null,null,null,29985,90551,"129_Sat May 13 2023 13:31:02 GMT+0800","2023-05-17T23:59:35","Observation","Ship Staff","Ship Staff Insp.","No.1 and 2 P/S TST  manhole cover lifting handle are corroded and wasted. require to renew","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","External Factors","","","",""," Renewal of  the manhole cover Lifting handle was completed.  ","2023-08-05T23:59:35","","Completed","2023-08-05T23:59:35","No","No","No","Internal"]
[null,null,null,30757,99360,"129_Mon Jun 05 2023 11:50:28 GMT+0800","2023-05-18T23:59:35","Defect","Ship Staff","Ship Staff Insp.","ME L.O Settling Tank#1&2 - Minor leakage from manhole cover.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Gasket renewed and damaged studs replaced with big size and internal thread damage repaired. Boxed back and taken oil in the tanks, found no leaks.","2023-06-01T23:59:35","","Completed","2023-05-22T23:59:35","No","No","No","Internal"]
[null,null,null,30758,14853,"129_Wed Jun 07 2023 07:36:43 GMT+0800","2023-05-18T23:59:35","Defect","Ship Staff","Ship Staff Insp."," Airline glove valve at portside between 3 &4 # on main deck wheel & spindle broken .","Deck - Pipe / Fittings","General Appearance","Equipment Related","","","",""," Airline glove valve at portside between 3 &4 # on main deck renewed. ","2023-05-19T23:59:35","","Completed","2023-05-19T23:59:35","No","No","No","Internal"]
[null,null,null,30760,96369,"129_Wed Jun 07 2023 15:32:17 GMT+0800","2023-05-19T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","ME LO Cooler S.W inlet pipe leaking from sealing face","E/R - Pipes/ valves & fittings,E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Action required: ME to stop and main C.S.W line to isolate for carrying out job. Need to replace the leaking pipe with spare fabricated pipe.\nAction taken: ME stopped for one hour, Main C.S.W line isolated and leaking pipe replaced with spare pipe with new gaskets.","2023-06-08T23:59:35","","Completed","2023-05-24T23:59:35","No","No","No","Internal"]
[null,null,null,30756,66263,"129_Mon Jun 05 2023 11:46:20 GMT+0800","2023-05-22T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","Vegetable room solenoid coil of magnet valve found not working, observed during daily rounds with high room temperature. ","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Spare recieved and solenoid valve renewed. Tried out and working satisfactory.","2023-08-17T23:59:35","CPHO230083","Completed","2023-07-19T23:59:35","No","No","No","Internal"]
[null,null,null,30759,54826,"129_Wed Jun 07 2023 07:50:04 GMT+0800","2023-05-22T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Weather tight door of Emg. Generator room rubber packing become rigid and stiff, loose the compression & not sitting properly. Rubber packing needs to renew.","Miscellaneous","General Appearance","External Factors","","","","","Weather tight door of Emg. Generator room rubber packing renewed. Ensured integrity by Chock test, found satisfactory.","2023-05-23T23:59:35","","Completed","2023-05-23T23:59:35","No","No","No","Internal"]
[null,null,null,31189,80519,"129_Sat Jul 01 2023 11:44:48 GMT+0800","2023-06-12T23:59:35","Defect","Ship Staff","Ship Staff Insp.","On Monkey Island battery room Gooseneck ventilation flap corroded and holed at bottom section. ","Accommodation","General Appearance","Equipment Related","","","","","Battery room Gooseneck ventilation flap corroded section renewed. ","2023-07-16T23:59:35","","Completed","2023-06-27T23:59:35","No","No","No","Internal"]
[null,null,null,31187,89576,"129_Fri Jul 07 2023 13:54:18 GMT+0800","2023-06-17T23:59:35","Defect","Ship Staff","Ship Staff Insp.","ME air cooler S.W inlet pipe has minor leak ","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","4 hours of stoppage permission required from office & Drain water from ME air cooler after isolation and do the hot work with office concurrence.","2023-07-17T23:59:35","","Completed","2023-06-23T23:59:35","No","No","No","Internal"]
[null,null,null,31185,50913,"129_Sat Jul 08 2023 11:59:15 GMT+0800","2023-06-21T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Received span gas on 03 oct 2023 at Singapore","Miscellaneous","Safety / LSA / FFA","Equipment Related","","","","","CPHO230053 has been raised accordingly.","2023-09-24T23:59:35","CPHO230053","Completed","2023-09-22T23:59:35","No","No","No","Internal","Items supplied in singapore"]
[null,null,null,31190,84502,"129_Sat Jul 08 2023 11:55:22 GMT+0800","2023-06-21T23:59:35","Defect","Ship Staff","Ship Staff Insp.","SOPEP Items are found out non-conformity with quantity. ","Miscellaneous","MARPOL Related","Equipment Related","","","","","All SOPEP items received CPHO230134 on 10 July at Singapore.","2023-07-02T23:59:35","CPHO230134","Completed","2023-06-26T23:59:35","No","No","No","Internal"]
[null,null,null,31191,27043,"129_Sat Jul 08 2023 11:57:19 GMT+0800","2023-06-21T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Onboard hydrometers are not working functionally.","Miscellaneous","General Appearance","Equipment Related","","","","","Received CPHO230126, new hydrometer on 10 July 2023, at singapore.","2023-07-02T23:59:35","CPHO230126","Completed","2023-06-26T23:59:35","No","No","No","Internal"]
[null,null,null,31188,95812,"129_Sat Jul 08 2023 11:46:25 GMT+0800","2023-06-24T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Shackles & turnbuckles used safety lines  near Rescue Boat & L/R were found out rusty and unable to turn.","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","Renewal of shackle/turnbuckle has been done. Satisfactory.  ","2023-06-30T23:59:35","","Completed","2023-06-24T23:59:35","No","No","No","Internal"]
[null,null,null,31192,73988,"129_Sat Jul 08 2023 11:44:58 GMT+0800","2023-06-24T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Most of Gas sampling points at Hatch Cover  are found out unable to turn. ","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","Proper maintenance has been  done to ensure all gas sampling points turnable properly. Satisfactory. ","2023-07-17T23:59:35","","Completed","2023-06-29T23:59:35","No","No","No","Internal"]
[null,null,null,31194,57487,"129_Sat Jul 08 2023 11:47:55 GMT+0800","2023-06-24T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Securing ropes used at hatch cover stopper pins are found out worn out / missing .  ","Miscellaneous","General Appearance","Equipment Related","","","","","Renewal of Securing ropes/wires at hatch cover stopper pins has been done. Satisfactory. ","2023-07-11T23:59:35","","Completed","2023-07-11T23:59:35","No","No","No","Internal"]
[null,null,null,31195,10231,"129_Wed Jul 12 2023 20:41:22 GMT+0800","2023-06-28T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Turnbuckles used securing for Freefall L/B Davit were found out rusty and unable to turn","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","Renewal of Turnbuckle has been done for ensuring turnable. Satisfactory. ","2023-08-17T23:59:35","","Completed","2023-07-11T23:59:35","No","No","No","Internal"]
[null,null,null,31198,35728,"129_Wed Jul 12 2023 20:42:47 GMT+0800","2023-06-28T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Rubber gasket for cargo hold access and cargo hold ventilation flap found out damaged.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","Renewal has be done. Satisfactory.  ","2023-08-17T23:59:35","","Completed","2023-08-02T23:59:35","No","No","No","Internal"]
[null,null,null,31197,67659,"129_Thu Jul 13 2023 12:19:07 GMT+0800","2023-06-29T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Most of butter fly nuts securing at Bobby Hatch Access were very hard to turn/secure. ","Deck - Pipe / Fittings","General Appearance","Equipment Related","","","","","Proper maintenance has be done for ensuring all nuts securing at cargo hold access able to turn/secure.  Satisfactory.   ","2023-08-17T23:59:35","","Completed","2023-07-26T23:59:35","No","No","No","Internal"]
[null,null,null,31193,68509,"129_Tue Jul 18 2023 22:49:39 GMT+0800","2023-06-30T23:59:35","Defect","Ship Staff","Ship Staff Insp.","WBT 4 (S) Vent head Cover  was found out damaged. ","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","Equipment Related","","","","","Rectified action (replacement of new wire mesh and cover) has been done accordingly. Satisfactory. ","2023-07-14T23:59:35","","Completed","2023-07-04T23:59:35","No","No","No","Internal"]
[null,null,null,29797,29893,"129_Thu Mar 30 2023 10:54:37 GMT+0800","2023-07-16T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Wire mesh of all gooseneck ventilators to be renewed. present wire mesh condition is broken or rusted.","Accommodation","Safety / LSA / FFA","External Factors,Human Error","","","","","All accomodation goose neck natural ventilation screen were renewed.","2023-09-24T23:59:35","CPHO230041","Completed","2023-10-01T23:59:35","No","No","No","Internal","CPHO230041 is supplied and closed. Please raise RO again for required items."]
[null,null,null,31196,21177,"129_Thu Aug 03 2023 00:27:41 GMT+0800","2023-07-19T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Missing Safety pin at Aft station working light frame  which can lead bulb damage. ","Deck - Pipe / Fittings","General Appearance","Equipment Related","","","","","Rectified action was taken immediately by fixing new safety pin. Satisfactory. ","2023-07-19T23:59:35","","Completed","2023-07-19T23:59:35","No","No","No","Internal"]
[null,null,null,31183,57785,"129_Wed Aug 09 2023 20:06:06 GMT+0800","2023-07-26T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Securing hook/point  at Freefall L/B was rusty and L/B Glass was dirty and vague ","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","Proper maintenance was done to ensure L/B glass be clean & transparent and no rusty at securing hook/point.  Good condition. ","2023-09-17T23:59:35","","Completed","2023-09-10T23:59:35","No","No","No","Internal"]
[null,null,null,31851,57743,"129_Mon Sep 04 2023 17:38:08 GMT+0800","2023-08-12T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Securing wires for Freefall L/B & Rescue boat  noted covering by fabric sheathing.","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","Removal of fabric sheathing has been done, wire condition was found out good condition. Applying greas was carried out. ","2023-08-26T23:59:35","","Completed","2023-08-22T23:59:35","No","No","No","Internal"]
[null,null,null,31849,92165,"129_Wed Sep 13 2023 15:30:57 GMT+0800","2023-08-22T23:59:35","Defect","Ship Staff","Ship Staff Insp.","During ME performance taken, was noted, ME Unit no.5, abnormal of low Pmax.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","M/E unit number 5 exhaust valve, fuel injectors and indicator valves renewed. Performance taken. Pmax is inline with other units.","2023-10-18T23:59:35","","Completed","2023-10-15T23:59:35","No","No","No","Internal","Please update the job, as it is completed."]
[null,null,null,31848,46401,"129_Wed Sep 13 2023 15:12:08 GMT+0800","2023-08-24T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Accommodation Ladder STB. - winch - gear box leakage from shaft's seals, due to worn out (over corroded) in sealing area. Oil leakage on deck, dropping.","Deck - Machinery","MARPOL Related","Equipment Related","","","","","Seal rings were renewed last overhauling and currently it is working satisfactory.","2023-10-18T23:59:35","CPHO230184","Completed","2023-08-28T23:59:35","No","No","No","Internal","PO is under processing."]
[null,null,null,31845,15367,"129_Wed Sep 13 2023 15:14:26 GMT+0800","2023-08-25T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Accommodation Ladder PS. - winch - gear box leakage from shaft's seals, due to worn out (over corroded) in sealing area. Oil leakage on deck, dropping.","Deck - Machinery","MARPOL Related","Equipment Related","","","","","Seal rings were renewed last overhauling and currently it is working satisfactory.","2023-10-18T23:59:35","CPHO230184","Completed","2023-08-27T23:59:35","No","No","No","Internal","PO is under processing."]
[null,null,null,31852,33833,"129_Wed Sep 13 2023 15:02:04 GMT+0800","2023-08-25T23:59:35","Defect","Ship Staff","Ship Staff Insp.","It was observed that slight crack on silicon around Freefall L/B External surface exhaust pipe.  ","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","Renewal of silicon has been done. Good condition.  ","2023-08-29T23:59:35","","Completed","2023-08-27T23:59:35","No","No","No","Internal"]
[null,null,null,31846,27246,"129_Fri Sep 08 2023 21:08:36 GMT+0800","2023-08-26T23:59:35","Defect","Ship Staff","Ship Staff Insp.","JRC MF-HF ANTENNA - ONE HORIZONTAL ANTENNA was found out missing out due to very strong wind.","Navigation - GMDSS & Communication","General Appearance","Equipment Related","","","","","Renewed antenna by service technician","2023-09-29T23:59:35","Renewed Antenna.","Completed","2023-09-22T23:59:35","No","No","No","Internal","Service technician attended in singapore"]
[null,null,null,31847,11411,"129_Wed Sep 13 2023 15:00:40 GMT+0800","2023-08-26T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Sea water pipe (elbow), inlet to ME jacket cooler, leakage.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Leak rectified. New pipe will fabricated in later date.","2023-10-18T23:59:35","","Completed","2023-10-08T23:59:35","No","No","No","Internal","Plan for the job at next suitable opportunity."]
[null,null,null,31850,88316,"129_Fri Sep 15 2023 16:47:19 GMT+0800","2023-09-02T23:59:35","Defect","Ship Staff","Ship Staff Insp.","During De-watering system testing , it was observed that F'cle Bosun's Store bilge well suction valve from Port side was stuck , very hard to turn properly and  water is not going out from Bosun's Store STBD bilge well.","Deck - Machinery","Structural Condn. / WT integrity ","Equipment Related","","","","","Both Bosun's store bilge well suction valves were removed , proper maintenance was performed . Once done, re-installation and De-watering system testing was carried out. Good condition.  ","2023-09-03T23:59:35","","Completed","2023-09-03T23:59:35","No","No","No","Internal","Update the job after completion."]
[null,null,null,31925,24031,"129_Tue Sep 26 2023 12:23:50 GMT+0800","2023-09-04T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Both Steering Gear Pumps, leakage from shaft seals. Due of very often, Bridge use both pump on, both pumps start to leakage from shaft seals, also some of the pipe leakage from o-rings.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Shore technician attended and overhauled. ","2024-01-23T23:59:35","","Completed","2024-01-23T23:59:35","No","No","No","Internal","Shore service attended and renewed the seal in singapore for No.2 steering gear pump. No.1 pump leak to be rectified. Spares already supplied to vessel."]
[null,null,null,31184,58896,"129_Sat Jul 08 2023 11:51:38 GMT+0800","2023-09-05T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Onboard items are found out non-compliance with SOLAS regulation  in quantity & quality. ( ( No steel toe type of Fireman boots/torn out , Only 2 Fireman walkie-talkies are available )","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","Has been received at singapore.","2023-11-19T23:59:35","CPHO230138","Completed","2024-01-23T23:59:35","No","No","No","Internal","Walkie talkies supplied at singapore. pls close the job."]
[null,null,null,31186,20396,"129_Fri Jul 14 2023 12:21:48 GMT+0800","2023-09-05T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Window wipers were not provided at bridge  front center screen for clear view, CVS was not fitted on front view of bridge","Miscellaneous","General Appearance","Equipment Related","","","","","SI instucted to remove from DDRL as this is not part of design.","2023-11-19T23:59:35","","Completed","2023-10-22T23:59:35","No","No","No","Internal","Pls remove this defect from DDRL as this is not part of the design."]
[null,null,null,31927,90962,"129_Tue Sep 26 2023 11:09:04 GMT+0800","2023-09-11T23:59:35","Defect","Ship Staff","Ship Staff Insp.","During weekly safety equipment round test, was found Search Light from Rescue Boat, bulb / lamp not lit, not working. Bulb / lamp is not bursted, is some loose contact inside, and sometime lit, sometime not. Not reliable.","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","Lamp received at Singapore port call. Same was installed and tried out, found working satisfactory.","2023-09-22T23:59:35","","Completed","2023-09-24T23:59:35","No","No","No","Internal","Item supplied in singapore"]
[null,null,null,31921,86532,"129_Tue Sep 26 2023 11:03:16 GMT+0800","2023-09-13T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","During normal sailing, AE no.2 online, AE no.3 stand by, low insulation 440V alarm occur. After investigation found, electric motor from Priming Pump (AE no.3), burn out. Motor or pump was moving very easy. Setting of safety in El. Panel, as per maker / yard, not any adjustment by crew.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","AE 3 LO priming pump motor received at Singapore. Motor renewed, tried-out and put into service.","2023-09-22T23:59:35","","Completed","2023-09-23T23:59:35","No","No","No","Internal","Item supplied in singapore"]
[null,null,null,31922,90311,"129_Tue Sep 26 2023 12:08:00 GMT+0800","2023-09-14T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Inlet sea water cooling pipe - tee, connected, one side to By-Pass vv- to the ME air cooler, leakage. Pipe need to be welded, or to fabricate new one.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","leaking pipe renewed with fabractaed pipe. leak rctified.","2023-11-19T23:59:35","","Completed","2023-10-06T23:59:35","No","No","No","Internal","Plan for the job at next suitable opportunity."]
[null,null,null,31923,16694,"129_Tue Sep 26 2023 12:13:03 GMT+0800","2023-09-14T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Main sea water cooling pipe, delivery pipe from Main Sea Water Pump no.1 -del vv & delivery pipe from Main Sea Water Pump no.2, del vv, to the main cooling sea water pipe line (tee pipe), leakage. Pipe need to be welded, or to fabricate new one.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","leaking pipe renewed with fabractaed pipe. leak rctified.","2023-11-19T23:59:35","","Completed","2023-10-25T23:59:35","No","No","No","Internal","Plan for the job at next suitable opportunity."]
[null,null,null,31924,53040,"129_Tue Sep 26 2023 12:17:34 GMT+0800","2023-09-14T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Sea water cooling pipe elbow inlet to ME lub oil cooler is leaking. Pipe / elbow to be welded.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","SW inlet line renewed with standby pipe.","2023-10-19T23:59:35","","Completed","2023-10-08T23:59:35","No","No","No","Internal","Plan for the job at next suitable opportunity."]
[null,null,null,31926,64038,"129_Fri Sep 29 2023 11:06:38 GMT+0800","2023-09-17T23:59:35","Defect","Ship Staff","Ship Staff Insp.","During Ballasting operations, was observed at BWTS PS, Back Flush Pump leakage from mechanical seal.  Also Sea Water Boster Pump minor leak from mechanical seal.","E/R - Pumps","Cargo / Ballast Systems","Equipment Related","","","","","Back flush pump casing cover oring renewed. Leak rectified. Booster Pump leak rectified.","2023-10-19T23:59:35","CPHO230142","Completed","2023-10-15T23:59:35","No","No","No","Internal","Items supplied in china. Pls update the job status"]
[null,null,null,32245,64405,"129_Wed Oct 11 2023 10:20:07 GMT+0800","2023-09-22T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","DG LT Cooler SW inlet pipe having leak at weld area","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Pipe replaced with reconditioned spare. Leak rectified.","2023-11-07T23:59:35","","Completed","2023-10-22T23:59:35","No","No","No","Internal","Plan to renew the pipe at next suitable opportunity."]
[null,null,null,32249,36880,"129_Wed Oct 11 2023 10:23:01 GMT+0800","2023-09-22T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","E/R Workshop curtain in poor condition","Miscellaneous","General Appearance","Inappropriate Procedure","","","","","Welding curtains renewed with recently received fire retardant type.","2023-09-29T23:59:35","","Completed","2023-09-25T23:59:35","No","No","No","Internal"]
[null,null,null,32250,72365,"129_Wed Oct 11 2023 10:29:29 GMT+0800","2023-09-22T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Chemical locker adjacent to Cyl Oil Storage tank found in disorder","Miscellaneous","General Appearance","Inappropriate Procedure","","","","","Area cleaned and all stained bulkheads painted new. Removed all garbage from the area.","2023-09-29T23:59:35","","Completed","2023-09-29T23:59:35","No","No","No","Internal"]
[null,null,null,32251,52806,"129_Wed Oct 11 2023 10:33:27 GMT+0800","2023-09-22T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","MGPS Flow meter found defected and most of the parts are wasted.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Recently received spares during Singapore port call. Flow meter was renewed and put into service.","2023-10-19T23:59:35","","Completed","2023-09-28T23:59:35","No","No","No","Internal"]
[null,null,null,32252,72962,"129_Wed Oct 11 2023 10:36:22 GMT+0800","2023-09-22T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Some bulkheads and air ducts at E/R casing are having stain marks.","Miscellaneous","General Appearance","Inappropriate Procedure","","","","","E/R casing area cleaned, all stain marks painted new.","2023-10-07T23:59:35","","Completed","2023-09-28T23:59:35","No","No","No","Internal"]
[null,null,null,32253,30143,"129_Wed Oct 11 2023 10:41:43 GMT+0800","2023-09-22T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Sludge pump pressure guge showing pressure even the pump is not running.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","","","","","Sludge pump line depressurized. Pressure gauge check and found working satisfactory.","2023-09-29T23:59:35","","Completed","2023-09-28T23:59:35","No","No","No","Internal"]
[null,null,null,32254,87558,"129_Wed Oct 11 2023 10:38:58 GMT+0800","2023-09-22T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Service air line found having leak from the drain line.","Deck - Pipe / Fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Leaking pipe section renewed.","2023-11-21T23:59:35","","Completed","2023-10-01T23:59:35","No","No","No","Internal"]
[null,null,null,32255,40291,"129_Wed Oct 11 2023 10:44:09 GMT+0800","2023-09-22T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Metal scraps found accumulated at steering gear room.","Miscellaneous","Eng. / Strg. Comp.","Inappropriate Procedure","","","","","Metal scraps to be landed at China","2023-10-23T23:59:35","","Completed","2023-10-08T23:59:35","No","No","No","Internal"]
[null,null,null,32256,91883,"129_Wed Oct 11 2023 10:48:42 GMT+0800","2023-09-30T23:59:35","Defect","Ship Staff","Ship Staff Insp.","M/E Air cooler de-earation line is leaking near the cooler.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Pipe leal rectified","2023-10-31T23:59:35","","Completed","2023-10-04T23:59:35","No","No","No","Internal"]
[null,null,null,32709,39572,"129_Sat Oct 28 2023 10:05:40 GMT+0800","2023-10-17T23:59:35","Defect","Ship Staff","Ship Staff Insp.","M/E unit No. 2 Fuel pump top cover leaking.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","M/E Fuel pump top cover Unit # 2 fuel pump top cover replaced with reconditioned spare. Leak rectified.","2023-12-21T23:59:35","","Completed","2023-10-23T23:59:35","No","No","No","Internal"]
[null,null,null,32707,60283,"129_Mon Oct 30 2023 09:54:15 GMT+0800","2023-10-19T23:59:35","Defect","Ship Staff","Ship Staff Insp.","M/E Air cooler SW pipe outlet has started to leak","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Temporarily repaired by clamp and reubber. RO CPHO230227 has been raised.\nNew pipe fabricated and fitted.","2023-12-21T23:59:35","CPHO230227","Completed","2023-11-20T23:59:35","No","No","No","Internal","Items will be supplied at Xiamen"]
[null,null,null,32708,14865,"129_Mon Oct 30 2023 09:51:35 GMT+0800","2023-10-19T23:59:35","Defect","Ship Staff","Ship Staff Insp.","M/E LO cooler SW outlet Pipe has started to leak.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Pipe renewed with newly fabricated one. Leak rectified.","2023-12-21T23:59:35","","Completed","2023-10-22T23:59:35","No","No","No","Internal"]
[null,null,null,33062,53262,"129_Wed Nov 29 2023 15:01:38 GMT+0800","2023-11-11T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Oxyzen and acetylene flexible hose are fitted with normal Jublee clamps. To replaced with approved type.","E/R - Pipes/ valves & fittings","ISM Related","Equipment Related","","","","","all hose clips were replaced with ear clamp clips.","2023-12-13T23:59:35","CPHO 230241","Completed","2023-11-20T23:59:35","No","No","No","Internal"]
[null,null,null,33060,94646,"129_Wed Nov 29 2023 14:56:59 GMT+0800","2023-11-13T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Stern Navigation Light casing has cracked very badly.","Elect. Mach. & Equip.","ISM Related","Equipment Related","","","","","New spare stern nav light casing received in china same fitted in position and tested out found to be working satisfactory.","2023-12-21T23:59:35","CPHO 230232 ","Completed","2023-11-23T23:59:35","No","No","No","Internal"]
[null,null,null,33063,78367,"129_Thu Nov 30 2023 10:55:34 GMT+0800","2023-11-13T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Main Eng unit-3 FO high pressure pipe fwd started to leak.","E/R - Main Engine","ISM Related","Equipment Related","","","","","Pipe overhauled and seal rings renewed.","2023-11-21T23:59:35","","Completed","2023-11-20T23:59:35","No","No","No","Internal"]
[null,null,null,33064,44840,"129_Wed Nov 29 2023 11:27:34 GMT+0800","2023-11-13T23:59:35","Defect","SIRE / CDI Insp.","Others (Eg. Insurance etc.)","To Apply LOCKTITE-5910 Between Stay bolt nut and mating surface A-Frame","E/R - Main Engine","Eng. / Strg. Comp.","External Factors","","","","","High-Temp RTV silicone applied on all M/E stay bolt hydraulic nuts bases.","2024-01-22T23:59:35","CPHO 230243","Completed","2023-12-04T23:59:35","No","No","No","External"]
[null,null,null,33061,83043,"129_Thu Nov 30 2023 10:53:29 GMT+0800","2023-11-16T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Main Eng unit-1 FO high pressur pipe (aft) started to leak.","E/R - Main Engine","ISM Related","Equipment Related","","","","","Pipe overhauled and seal rings renewed.","2023-11-21T23:59:35","","Completed","2023-11-20T23:59:35","No","No","No","Internal"]
[null,null,null,33656,99795,"129_Wed Jan 10 2024 08:42:48 GMT+0800","2023-12-03T23:59:35","Defect","Ship Staff","Ship Staff Insp.","M/E electrical-pneumatic manoeuvering system Quick release valve (pos 124) for puncture valve air line found leaking. Upon opening, found rubber diapragm damage (installed already with fabriacted diapragm made by previous staffs).","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Valve has been renewed with spare. Now working satisfactory.","2024-03-02T23:59:35","CPHO230249","Completed","2024-02-12T23:59:35","No","No","No","Internal","Spare part supplied at singapore. Pls renew at next opportunity."]
[null,null,null,33057,63950,"129_Fri Dec 15 2023 15:18:28 GMT+0800","2023-12-06T23:59:35","Defect","Ship Staff","Ship Staff Insp.","E/R Cofferdam vent head (STBD) found wasted and beyond repair.","Hull & Tanks","Structural Condn. / WT integrity ","Equipment Related","","","","","Vent head has been replaced.","2024-03-06T23:59:35","CPHO230251","Completed","2024-02-22T23:59:35","No","No","No","Internal","PO placed. Will be supplied at next port."]
[null,null,null,33652,14308,"129_Wed Dec 20 2023 20:01:38 GMT+0800","2023-12-12T23:59:35","Defect","Ship Staff","Ship Staff Insp.","NRV of Master valve for Cargo hold bilges have play and which could result in SW getting leaked into the Cargo holds.","Cargo Mach.,E/R - Pipes/ valves & fittings","Cargo / Ballast Systems","Equipment Related","","","","","Valve has been renewed.","2024-03-02T23:59:35","CPHO230246","Completed","2024-01-27T23:59:35","No","No","No","Internal","Spare valve supplied in korea. Pls renew."]
[null,null,null,33659,41021,"129_Wed Jan 03 2024 13:30:52 GMT+0800","2023-12-13T23:59:35","Observation","FSC Inspector","Others (Eg. Insurance etc.)","Engine control room temperatures is high. \nAs per AMSPEC Safety Vetting Insepection report last Dec 21, 2023.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","ECR package AC unit evaporator and condenser were cleaned. Unit charged with Refrigerant.  AC performance improved and found satisfactory.","2024-02-24T23:59:35","","Completed","2023-12-18T23:59:35","No","No","No","External"]
[null,null,null,33658,62374,"129_Wed Jan 03 2024 17:28:00 GMT+0800","2023-12-14T23:59:35","Observation","Others (Eg. Insurance etc.)","Others (Eg. Insurance etc.)","Draft guages of port and stbd side are not matching with each other and also not matching with visual drafts. fwd and aft draft guages have differnce of 30cms.","Hull & Tanks","Cargo / Ballast Systems","Equipment Related","","","","","fault finding carried out, port and stbd sensors inspected and cleaned, sensor output curernt singals checked, zero calibration done for the same rectified the fault, now the draft gauges are working satisfactory.","2024-03-22T23:59:35","","Completed","2024-01-18T23:59:35","No","No","No","Internal","Carry out troubleshooting and send the updates."]
[null,null,null,33653,35275,"129_Fri Dec 29 2023 08:39:26 GMT+0800","2023-12-20T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Sea Water Pipe is leaking, located between Emg. Bilge suction and No. 1 Main CWS Pump.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Pipe has been renewed. Now good condition.","2024-03-21T23:59:35","","Completed","2024-01-26T23:59:35","No","No","No","Internal","Update the job after completion."]
[null,null,null,33654,32510,"129_Thu Dec 28 2023 20:12:56 GMT+0800","2023-12-20T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Valve no 001,003 and 006  not operational from CCR.","Hull & Tanks,E/R - Pipes/ valves & fittings","Cargo / Ballast Systems","Equipment Related","","","","","valve motors have been overhauled, valve actuators opening and closing checked, trouble shooting carried out for the same and tested out from CCR found to be working","2024-06-22T23:59:35","","Completed","2024-01-16T23:59:35","No","No","No","Internal","Carry out troubleshooting and send the updates. Create RO for required spares."]
[null,null,null,34024,60158,"129_Mon Feb 12 2024 01:19:07 GMT+0800","2024-01-22T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","All ballast tank manholes on deck to be derusted and painted.","Hull & Tanks","General Appearance","External Factors","","","","","Manholes on deck have been derusted and painted.","2024-03-22T23:59:35","","Completed","2024-03-06T23:59:35","No","No","No","Internal","Plan the job during loaded passage."]
[null,null,null,34025,73611,"0_Mon Feb 12 2024 01:14:23 GMT+0800","2024-01-22T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Meat room fan is making abnormal noise. To overhaul the fan.","Accommodation","Safety / LSA / FFA","Equipment Related","","","","","Inspected the meat room fan, Fan is making noise because blocking inside evaporator coil by frost. Defrosted evaporator coil thoroughly, fan is in good condition and there is no abnormal noise.","2024-02-22T23:59:35","","Completed","2024-02-11T23:59:35","No","No","No","Internal","Noted. Check the required spares before overhauling the motor."]
[null,null,null,34026,24888,"0_Mon Feb 12 2024 01:23:32 GMT+0800","2024-01-22T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Main engine Spare cylinder cover to be assembled with exhaust valve, air starting valve and fuel valves.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Spare cylinder cover has been assembled with exhaust valve, air starting valve and fuel valves.","2024-02-22T23:59:35","","Completed","2024-02-06T23:59:35","No","No","No","Internal"]
[null,null,null,34027,48474,"0_Mon Feb 12 2024 01:21:26 GMT+0800","2024-01-22T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Paint locker to be arranged properly","Miscellaneous","General Appearance","External Factors","","","","","Paint locker has been arranged.","2024-02-08T23:59:35","","Completed","2024-02-06T23:59:35","No","No","No","Internal"]
[null,null,null,34030,97868,"129_Mon Feb 12 2024 01:05:01 GMT+0800","2024-01-22T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Crew laundry door closer is not working properly.","Accommodation","Structural Condn. / WT integrity ","External Factors","","","","","Door closer has been repaired, now good condition.","2024-02-08T23:59:35","","Completed","2024-02-07T23:59:35","No","No","No","Internal"]
[null,null,null,34031,20113,"0_Mon Feb 12 2024 01:25:36 GMT+0800","2024-01-22T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","No.2 ME FO circulating pump suction pressure gauge to be renewed with higher range pressure gauge.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","","","","","Pressure gauge has been renewed with higher range pressure gauge.","2024-02-08T23:59:35","","Completed","2024-02-05T23:59:35","No","No","No","Internal"]
[null,null,null,34028,76713,"129_Fri Feb 16 2024 01:09:20 GMT+0800","2024-02-05T23:59:35","Observation","Ship Staff","Ship Staff Insp.","No.1 A/E L.O priming pump motor having abnormal sound.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","L.O priming pump motor has been overhauled, renewed both bearings. Now good condition.","2024-02-12T23:59:35","","Completed","2024-02-06T23:59:35","No","No","No","Internal"]
[null,null,null,34029,41550,"129_Fri Feb 16 2024 01:11:12 GMT+0800","2024-02-05T23:59:35","Observation","Ship Staff","Ship Staff Insp.","No.2 A/E L.O priming pump motor having abnormal sound.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","L.O priming pump motor has to be overhauled, renewed both bearings. Overhauled pump, renewed shaft. Now good condition.","2024-02-12T23:59:35","","Completed","2024-02-07T23:59:35","No","No","No","Internal"]
[null,null,null,34710,11831,"129_Fri Mar 15 2024 16:56:08 GMT+0800","2024-02-27T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Aft remote draft gauge showing erratic value.","Elect. Mach. & Equip.","Cargo / Ballast Systems","Equipment Related","","","","","Fault finding carried out, sensors inspected and cleaned. Checked Transmitter outpur current, showing error. Renewed Transmitter, and monitored. Now working normal.","2024-05-12T23:59:35","","Completed","2024-05-05T23:59:35","No","No","No","Internal","Noted. Carry out troubleshooting once the loop calibrator is available."]
[null,null,null,34711,74984,"129_Fri Mar 08 2024 02:14:21 GMT+0800","2024-02-29T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Water leakage form Hot water circulating pump gland packing.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","","","","","Hot water circulating pump gland packing has been checked and renewed, pump derusted, Painted.","2024-03-04T23:59:35","","Completed","2024-03-01T23:59:35","No","No","No","Internal"]
[null,null,null,34731,65342,"129_Sat Mar 30 2024 16:54:44 GMT+0800","2024-03-11T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Accom ladder (STBD side) cannot be operated due to selector switch defective.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","Selector switch has been renewed with spare. Now normal working condition.","2024-04-26T23:59:35","CPHO240079","Completed","2024-04-19T23:59:35","No","No","No","Internal","PO is under processing. Will be supplied at port cartier."]
[null,null,null,34732,48186,"129_Sat Mar 30 2024 16:43:50 GMT+0800","2024-03-20T23:59:35","Observation","Ship Staff","Ship Staff Insp.","MGPS SW line slight leak from flange.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Leakage rectified.","2024-03-25T23:59:35","","Completed","2024-03-21T23:59:35","No","No","No","Internal"]
[null,null,null,35003,39160,"129_Mon Apr 15 2024 18:15:32 GMT+0800","2024-04-01T23:59:35","Observation","Ship Staff","Ship Staff Insp.","ME CSW line found pin hole and leaking.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Removed the pipe from place and repaired, pipe cleaned inside and applied two coat of epoxy primer . Fitted back with new gasket.","2024-04-08T23:59:35","","Completed","2024-04-06T23:59:35","No","No","No","Internal"]
[null,null,null,33655,65608,"129_Wed Jan 03 2024 13:40:28 GMT+0800","2024-04-28T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Navigation bridge temperatures is high.\nAs per AMSPECT safety vetting inspection report last Dec 21, 2023","Miscellaneous","Structural Condn. / WT integrity ","Equipment Related","","","","","New AC unit received and installed by shore service team.","2024-06-27T23:59:35","CPHO230239 SPLIT AIR CONDITIONING SYSTEM FOR BRIDGE","Completed","2024-06-16T23:59:35","No","No","No","Internal","PO is under processing. New unit will be supplied at next suitable port."]
[null,null,null,35818,57739,"129_Fri May 10 2024 14:40:08 GMT+0800","2024-05-02T23:59:35","Observation","Ship Staff","Ship Staff Insp.","CH bilge educting master globe valve body cracked(5K-125).","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","New valve recived and replaced on 29.06.2024","2024-06-27T23:59:35","CPHO240101 - CARGO HOLD BILGE EDUCTOR VALVE","Completed","2024-06-27T23:59:35","No","No","No","Internal","New valve will be supplied in china."]
[null,null,null,35819,97677,"129_Fri May 10 2024 14:17:46 GMT+0800","2024-05-03T23:59:35","Observation","Ship Staff","Ship Staff Insp."," Found incinerator furnace refractory damaged.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","",""," Incinerator furnace refractory patch up work carried.","2024-05-11T23:59:35","","Completed","2024-05-04T23:59:35","No","No","No","Internal"]
[null,null,null,35820,64322,"129_Tue May 28 2024 21:47:40 GMT+0800","2024-05-24T23:59:35","Observation","Ship Staff","Ship Staff Insp.","FWG ejector pump suction line found pin hole and leaking.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Pipe removed and repaired, fabricated, leak rectified.","2024-05-28T23:59:35","","Completed","2024-05-25T23:59:35","No","No","No","Internal"]
[null,null,null,36228,42437,"129_Sat Jun 15 2024 16:26:00 GMT+0800","2024-06-09T23:59:35","Observation","Ship Staff","Ship Staff Insp.","ME cooling S.W pipe pin hold leak.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Removed the pipe from place and repaired, pipe cleaned inside and applied two coat of epoxy primer . Fitted back with new gasket.","2024-06-15T23:59:35","","Completed","2024-06-12T23:59:35","No","No","No","Internal"]
[null,null,null,null,11610,"129_Fri Jul 05 2024 17:57:20 GMT+0800","2024-07-02T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Generator No.1 and Generator No.3 Turbocharger inlet temperature sensor is malfunctioning.","E/R - Aux. Engine","","Equipment Related","","","","","New sensors were received in china, sensors were fitted in place and temeperatures monitored found to be working satisfactory.","2024-08-04T08:00:00","CPHO240152","Completed","2024-08-05T08:00:00","No","No","No","Internal","Order already placed by NGM."]
[null,null,null,null,67514,"129_Wed Apr 05 2023 23:06:41 GMT+0800","2024-04-28T08:00:00","Critical Equipment,Non Conformity,Defect","Ship Staff","Nav Audit / Verification","Doppler log showing erratic readings on screen. No STW available for Collision avoidance.","Navigation - Echo Sounder / Speed Log","Navigation","Equipment Related","","","","","New transducer was renewed in singapore on JAN-2024, instructions were received from office regarding the XDCR settings, settings was changed by the ship staff accordingly and doppler log found to be working satisfactory.","2024-07-29T08:00:00","","Completed","2024-04-30T08:00:00","No","No","No","Internal","New transducer supplied by maker., same to be replaced at next opportunity."]
[null,null,null,null,91518,"129_Wed Oct 11 2023 11:00:44 GMT+0800","2024-06-28T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Aux. CSW line to DG LT cooler is leaking at tank top inside bilges.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","This is a MCSW pump discharge manifold pipe.\nPlan for the job at next suitable opportunity.\nThis repair job of the manifold pipe line required new fabrication of all the poor condition sections of the branch pipes of the discharge manifold.\nAnd Also required to go for a black out to remove and replace the pipe lines as isolation of the system is not possible other than stopping the both MCSW pumps.\nAbout 4m length Pipe Located at the bottom of the E/R bilges. Acsess to the deffective pipe is difficalt. Remove and taking out deffective pipe line required to remove the other pipe lines which are on top the deffective line. Also required  to cut the bildge floor brackets & angle bar supports. Need Ample time and a Workshop assistance.\n================================================================\nJob completed by shore workshop at XIAMEN Anchorage","2024-09-28T08:00:00","CPHO230201","Completed","2024-08-02T08:00:00","Yes","No","No","Internal","Shore workshop arranged for repairs in China."]
[null,null,null,null,17003,"129_Wed Oct 11 2023 10:57:27 GMT+0800","2024-06-28T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Interconnection SW pipe between Main CSW and Aux CSW line is leaking at tank top, inside bilges.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","This is a MCSW pump discharge manifold pipe.\nPlan for the job at next suitable opportunity.\nThis repair job of the manifold pipe line required new fabrication of all the poor condition sections of the branch pipes of the discharge manifold.\nAnd Also required to go for a black out to remove and replace the pipe lines as isolation of the system is not possible other than stopping the both MCSW pumps.\nPipe Located at the bottom of the E/R bilges. Acsess to the deffective pipe is difficalt. Remove and taking out deffective pipe line required to remove the other pipe lines which are on top the deffective line. Also required  to cut the bildge floor brackets & angle bar supports. Need Ample time and a Workshop assistance.\n================================================================\nJob completed by shore workshop at XIAMEN Anchorage","2024-09-28T08:00:00","","Completed","2024-08-02T08:00:00","Yes","No","No","Internal","Shore workshop arranged for repairs"]
[null,null,null,null,88076,"129_Wed Oct 11 2023 10:53:36 GMT+0800","2024-06-28T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Aux CSW line inlet to Atmospheric Condenser is leaking.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Plan to carry out at suitable opportunity.This repair job of the manifold pipe line required new fabrication of all the poor condition sections of the branch pipes of the discharge manifold.\nAnd Also required to go for a black out to remove and replace the pipe lines as isolation of the system is not possible other than stopping the both MCSW pumps. The pipe line which is temporary repaired by means of plastic steel leads to the DG LT coolers,  blackout cannot be avoided anyway.\nAbout 5m length pipe at the E/R bilges. Acsess difficult. Required to cut the bildge floor brackets & angle bar supports. Need Ample time and a Workshop assistance.\n================================================================\nJob completed by shore workshop at XIAMEN Anchorage","2024-09-28T08:00:00","","Completed","2024-08-02T08:00:00","No","No","No","Internal","Shore workshop arranged for repairs"]
[null,null,null,null,35236,"129_Thu Aug 15 2024 22:11:09 GMT+0800","2024-08-12T08:00:00","Breakdown","Ship Staff","Ship Staff Insp.","BWMS ELECTROLYSIS UNIT DOSING PUMP BEARING DAMAGED WHILE IN SERVICE. PUMP OUT OF ORDER.","E/R - Pumps","","Equipment Related","","","","","DAMAGED PUMP REPLACED WITH NEW ONE","2024-09-15T08:00:00","RO - CPHO240190 RAISED IN PAL","Completed","2024-08-29T08:00:00","No","No","No","Internal"]
[null,null,null,null,19566,"129_Thu Aug 15 2024 14:21:26 GMT+0800","2024-08-13T08:00:00","Breakdown","Ship Staff","Ship Staff Insp.","BWMS #2 PORT SIDE SYSTEM TRO PNUMATIC PUMP DEFFECTIVE","E/R - Pumps","Cargo / Ballast Systems","Equipment Related","","","","","AIR OPERATED DEFFECTIVE PNUMATIC PUMP REPLACED WITH NEW ONE ","2024-09-13T08:00:00","RO - CPHO240191 RAISED IN PAL","Completed","2024-08-30T08:00:00","No","No","No","Internal"]
[null,null,null,null,49820,"129_Fri Sep 13 2024 08:34:04 GMT+0800","2024-09-13T08:00:00","Defect","Ship Staff","Ship Staff Insp.","AE #1 cannot take full load. As of now able to take about 50% of load. \nTurbocharger exhaust gas inlet goes beyond 500 Deg. C when increasing load more than 50%.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","T/C cartridge major overhaul carried out with bearing renewal. \nNozzle ring replaced with new one. AE #1 ABLE take full sea load.  Performance taken and found satisfactory operation.","2024-10-15T08:00:00","Requisition  CPHO240181  received.","Completed","2024-10-14T08:00:00","No","No","No","Internal"]

{"sheet":"Calc","index":2,"n_rows":28,"n_cols":12,"rows_kept":28,"cut":false,"hidden":true,"merged":[]}
["Def_type","Def_cause","Equipments","VIQrefno","Observer_code"]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,"Dim itemSele As Long"]
[null,null,null,null,null,null,null,null,null,null,null,"   dim startRow as integer"]
[null,null,null,null,null,null,null,null,null,null,null,"   startRow=1"]
[null,null,null,null,null,null,null,null,null,null,null,"        For itemSele = 0 To ListBox1.ListCount - 1"]
[null,null,null,null,null,null,null,null,null,null,null,"        If ListBox1.Selected(itemSele) = True Then"]
[null,null,null,null,null,null,null,null,null,null,null,"        Worksheets(\"WorksheetName\").Range(\"A\" & startRow).Value = ListBox1.List(itemSele)"]
[null,null,null,null,null,null,null,null,null,null,null,"        startRow = startRow + 1"]
[null,null,null,null,null,null,null,null,null,null,null,"        End If"]
[null,null,null,null,null,null,null,null,null,null,null,"        Next"]
[null,null,null,null,null,null,null,null,null,null,null,"Dim LastRowA As String"]
[null,null,null,null,null,null,null,null,null,null,null,"        Dim itemSele As Long"]
[null,null,null,null,null,null,null,null,null,null,null,"       Dim startRow as integer"]
[null,null,null,null,null,null,null,null,null,null,null,"        LastRowA = ActiveSheet.Cells(Rows.count, \"A\").End(xlUp).row"]
[null,null,null,null,null,null,null,null,null,null,null,"        startQue = 0"]
[null,null,null,null,null,null,null,null,null,null,null,"        For itemSele = 0 To ListBox1.ListCount - 1"]
[null,null,null,null,null,null,null,null,null,null,null,"        For startRow = 1 To LastRowA"]
[null,null,null,null,null,null,null,null,null,null,null,"        If Worksheets(\"WorksheetName\").Range(\"A\" & startRow).Value = ListBox1.List(itemSele) Then"]
[null,null,null,null,null,null,null,null,null,null,null,"        ListBox1.Selected(itemSele) = True"]
[null,null,null,null,null,null,null,null,null,null,null,"        Exit For"]
[null,null,null,null,null,null,null,null,null,null,null,"        End If"]
[null,null,null,null,null,null,null,null,null,null,null,"        Next j"]
[null,null,null,null,null,null,null,null,null,null,null,"        Next"]
[null,null,null,null,null,null,null,null,null,null,null,"        End If"]

{"sheet":"Areaofobs","index":3,"n_rows":17,"n_cols":2,"rows_kept":17,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Cargo / Ballast Systems",11]
["Cert. & Docu.",2]
["Communication",6]
["Crew Management",3]
["Emgcy. Systems",13]
["Eng. / Strg. Comp.",14]
["General Appearance",15]
["Ice Opns.",17]
["ISM Related",7]
["ISPS Related",10]
["MARPOL Related",9]
["MLC Related",4]
["Mooring",12]
["Navigation",5]
["Safety / LSA / FFA",8]
["Structural Condn. / WT integrity ",16]

{"sheet":"Vessel_type","index":4,"n_rows":1,"n_cols":2,"rows_kept":1,"cut":false,"hidden":true,"merged":[]}
["Vessel_type","ID"]

{"sheet":"Deficiency_type","index":5,"n_rows":8,"n_cols":3,"rows_kept":8,"cut":false,"hidden":true,"merged":[]}
["TITLE","Type of deficiency_description","ID"]
["Breakdown",null,6]
["Critical Equipment",null,4]
["Defect",null,1]
["Guarantee Claim",null,8]
["Non Conformity",null,2]
["Observation",null,3]
["Other",null,7]

{"sheet":"VIQrefno","index":6,"n_rows":1,"n_cols":3,"rows_kept":1,"cut":false,"hidden":true,"merged":[]}
["VIQ_ref_no","Risk Value of observation","ID"]

{"sheet":"Equipment_list","index":7,"n_rows":28,"n_cols":3,"rows_kept":28,"cut":false,"hidden":true,"merged":[]}
["TITLE","Equipment_list_description","ID"]
["Accommodation",null,12]
["Cargo Mach.",null,13]
["Critical Equip.",null,16]
["Deck - Machinery",null,18]
["Deck - Mooring Machinery",null,15]
["Deck - Pipe / Fittings",null,20]
["Documentation",null,21]
["E/R - Air Comp.",null,8]
["E/R - Aux. Engine",null,4]
["E/R - Aux. Mach.",null,7]
["E/R - Boiler",null,5]
["E/R - Main Engine",null,3]
["E/R - Pipes/ valves & fittings",null,9]
["E/R - Pumps",null,32]
["E/R - Purifier",null,6]
["Elect. Mach. & Equip.",null,10]
["Hull & Tanks",null,19]
["Inert Gas",null,14]
["LSA / FFA",null,17]
["Miscellaneous",null,22]
["Navigation - DGPS / EPFS / AIS",null,28]
["Navigation - ECDIS",null,25]
["Navigation - Echo Sounder / Speed Log",null,26]
["Navigation - GMDSS & Communication",null,23]
["Navigation - Others",null,11]
["Navigation - RADAR",null,24]
["Navigation - VDR / BNWAS",null,30]

{"sheet":"PSC_MOU","index":8,"n_rows":11,"n_cols":3,"rows_kept":11,"cut":false,"hidden":true,"merged":[]}
["TITLE","PSC_MOU_description","ID"]
["Asia and the Pacific",null,2]
["Caribbean",null,4]
["Europe and the North Atlantic",null,1]
["Latin America",null,3]
["The Black Sea region",null,6]
["The Indian Ocean",null,8]
["The Mediterranean",null,7]
["The Riyadh MoU",null,9]
["USCG",null,10]
["West and Central Africa",null,5]

{"sheet":"Inspection_type","index":9,"n_rows":13,"n_cols":2,"rows_kept":13,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Bunkering Audit",14]
["Cargo Audit",17]
["Engineering Audit",16]
["ISM Audit",2]
["ISPS Audit",3]
["IT Audit",10]
["MLC Audit",1]
["Mooring Audit",9]
["Nav Audit / Verification",8]
["Onboard Training",18]
["Ship Staff Insp.",15]
["Suptd. Insp.",13]

{"sheet":"Deficiency_Cause","index":10,"n_rows":8,"n_cols":3,"rows_kept":8,"cut":false,"hidden":true,"merged":[]}
["TITLE","Deficiency_Cause_description","ID"]
["Behaviour Based",null,1]
["Equipment Related",null,4]
["External Factors",null,5]
["Human Error",null,7]
["Inappropriate Procedure",null,8]
["Industry Issue",null,6]
["Knowledge Based",null,3]

{"sheet":"Observer_code","index":11,"n_rows":3,"n_cols":3,"rows_kept":3,"cut":false,"hidden":true,"merged":[]}
["TITLE","Observer_code_description","ID"]
["Owner / Marine / Tech. Suptd.",null,3]
["Ship Staff",null,2]

{"sheet":"Status_code","index":12,"n_rows":6,"n_cols":3,"rows_kept":6,"cut":false,"hidden":true,"merged":[]}
["TITLE","Status_code_description","ID"]
["Completed",null,6]
["Deferred to D D",null,5]
["In progress",null,3]
["Not Started",null,2]
["Waiting spare",null,4]

{"sheet":"PSC_ref_no","index":13,"n_rows":19,"n_cols":2,"rows_kept":19,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Alarms",9]
["Cargo operations including equipment",7]
["Certificates & Documentation",2]
["Dangerous Goods",13]
["Emergency Systems",5]
["Fire safety",8]
["ISM",16]
["ISPS",17]
["Life saving appliances",12]
["MLC, 2006",18]
["Other",19]
["Pollution Prevention",15]
["Propulsion and auxiliary machinery",14]
["Radio communication",6]
["Safety of Navigation",11]
["Structural condition",3]
["Water/Weathertight condition",4]
["Working and Living Conditions",10]

{"sheet":"Risk_value_of_obs","index":14,"n_rows":1,"n_cols":2,"rows_kept":1,"cut":false,"hidden":true,"merged":[]}
["Risk Value of observation","ID"]

{"sheet":"Year","index":15,"n_rows":18,"n_cols":1,"rows_kept":18,"cut":false,"hidden":true,"merged":[]}
["Year"]
[2014]
[2015]
[2016]
[2017]
[2018]
[2019]
[2020]
[2021]
[2022]
[2023]
[2024]
[2025]
[2026]
[2027]
[2028]
[2029]
[2030]

{"sheet":"Month","index":16,"n_rows":13,"n_cols":1,"rows_kept":13,"cut":false,"hidden":true,"merged":[]}
["Month"]
["Jan"]
["Feb"]
["Mar"]
["Apr"]
["May"]
["Jun"]
["Jul"]
["Aug"]
["Sep"]
["Oct"]
["Nov"]
["Dec"]

{"sheet":"Date_","index":17,"n_rows":32,"n_cols":1,"rows_kept":32,"cut":false,"hidden":true,"merged":[]}
["Date"]
["01"]
["02"]
["03"]
["04"]
["05"]
["06"]
["07"]
["08"]
["09"]
[10]
[11]
[12]
[13]
[14]
[15]
[16]
[17]
[18]
[19]
[20]
[21]
[22]
[23]
[24]
[25]
[26]
[27]
[28]
[29]
[30]
[31]

{"sheet":"Sheet1","index":18,"n_rows":24,"n_cols":6,"rows_kept":24,"cut":false,"hidden":true,"merged":[]}
[]
[null,"ID","E",null,"Date Recorded",1]
[null,"UNIQUE ID","F",null,"Type of Deficiency",2]
[1,"Date Recorded","G",null,"Observer code",3]
["ignore","Vessel Type","H",null,"Type of Inspection",4]
[null,"Internal / External","I",null,"Description of Deficiency",5]
[null,"Drydock","J",null,"Equipment Categories",6]
[null,"Information Sharing","K",null,"Area of Observation",7]
[null,"Critical_item","L",null,"Deficiency Cause",8]
[null,"Deficiency Type","M",null,"VIQ Ref Number",9]
[null,"Deficiency Cause","N",null,"Risk Value of Obs",10]
[null,"Inspection Type","O",null,"PSC Ref Number",11]
[null,"Equipments","P",null,"PSC MOU ID",12]
[null,"VIQ Reference Number","Q",null,"Action Taken or Required",13]
[null,"Risk Value of the observation","R",null,"Target Date",14]
[null,"PSC Reference Number","S",null,"PO Ref No.",15]
[null,"PSC MOU","T",null,"Status Code",16]
[null,"Observer Code","U",null,"Date Completed",17]
[null,"Target Date","V",null,"Drydock",18]
[null,"Status Code","W",null,"Info Sharing",19]
[null,"Description of Deficiency","X",null,"Critical Item Flag",20]
[null,"Action taken / required","Y",null,"Audit Type",21]
[null,"PO ref no","Z"]
[null,"Date completed","AA"]

{"sheet":"Ship_information","index":19,"n_rows":2,"n_cols":3,"rows_kept":2,"cut":false,"hidden":true,"merged":[]}
["Ship_ID","Ship_Name","FILE_NAME"]
["129","CAPE PHOENIX (11-08-2024)","129_1723349389744.xlsm"]

{"sheet":"External_Deficiency_type","index":20,"n_rows":5,"n_cols":3,"rows_kept":5,"cut":false,"hidden":true,"merged":[]}
["TITLE","Type of deficiency_description","ID"]
["Condn of Class / Memo",null,5]
["Defect",null,1]
["Non Conformity",null,2]
["Observation",null,3]

{"sheet":"External_Inspection_type","index":21,"n_rows":11,"n_cols":2,"rows_kept":11,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Cargo Audit",17]
["Flag State Insp.",5]
["ISM Audit",2]
["ISPS Audit",3]
["MLC Audit",1]
["Nav Audit / Verification",8]
["OM Insp. (Eg. SIRE / CDI etc.)",6]
["Others (Eg. Insurance etc.)",12]
["PSC Inspection",4]
["Terminal Insp.",11]

{"sheet":"External_Observer_code","index":22,"n_rows":7,"n_cols":3,"rows_kept":7,"cut":false,"hidden":true,"merged":[]}
["TITLE","Observer_code_description","ID"]
["Class Surveyor",null,4]
["FSC Inspector",null,5]
["Others (Eg. Insurance etc.)",null,9]
["PSC Insp.",null,6]
["SIRE / CDI Insp.",null,8]
["Terminal Insp.",null,7]

{"sheet":"Sheet Version","index":23,"n_rows":2,"n_cols":2,"rows_kept":2,"cut":false,"hidden":true,"merged":[]}
["Version","Title"]
["2.0","Version 2.0"]