{"text_format":"1","workbook":"xlsx","n_sheets":24,"sheets":["Mainsheet","Completed","Calc","Areaofobs","Vessel_type","Deficiency_type","VIQrefno","Equipment_list","PSC_MOU","Inspection_type","Deficiency_Cause","Observer_code","Status_code","PSC_ref_no","Risk_value_of_obs","Year","Month","Date_","Sheet1","Ship_information","External_Deficiency_type","External_Inspection_type","External_Observer_code","Sheet Version"],"not_rendered":{"charts":0,"images":1,"macros":1,"external_links":0,"defined_names":12,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Mainsheet","index":0,"n_rows":28,"n_cols":28,"rows_kept":28,"cut":false,"hidden":false,"merged":[[10,8,10,9],[10,12,10,13],[12,6,12,27],[8,6,8,27]]}
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,"Defect - Damage Monitoring Sheet"]
[]
[null,null,null,null,null,null,null,"Date of Report","30-Apr-2025",null,null,"Ship Name","DHT PEONY (17-02-2025)"]
[]
[null,null,null,null,null,null,"VERSION : 2.0"]
[]
[]
[]
[null,null,null,"ID","SHIPSIDE UNIQUEID","UNIQUE ID","Date Recorded","Type of Deficiency","Observer code","Type of Inspection","Description of Deficiency","Equipment Categories","Area of Observation","Deficiency Cause","VIQ Ref Number","Risk Value of Obs","PSC Ref Number","PSC MOU ID","Action Taken or Required","Target Date","PO Ref No.","Status Code","Date Completed","Drydock","Info Sharing","Critical Item","Audit Type","Superintendent Remarks"]
[null,null,null,null,55998,"50_Sat Aug 19 2023 11:55:31 GMT+0800","2023-08-01T08:00:00","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","COW Lines U Bolts corroded and wasted at various locations.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","11.1","High","","","Main COW line U bolts derusting and painting completed, Branch COW lines derusting and painting in progress","2025-05-30T08:00:00","","In progress",null,"No","No","No","Internal"]
[null,null,null,null,53693,"50_Sun Sep 29 2024 04:30:47 GMT+0800","2024-06-15T08:00:00","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Numerous pipe supports on main deck to derust and paint","Deck - Pipe / Fittings","","Equipment Related","","","","","Pipe supports on main deck to derusting and painting in progress","2025-05-30T08:00:00","","In progress",null,"No","No","No","Internal"]
[null,null,null,null,85008,"0_Mon Jul 15 2024 23:39:15 GMT+0800","2024-07-05T08:00:00","Observation","Ship Staff","Ship Staff Insp.","The loadicator draft  does not match with the visual drafts.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","It was observed that the loadicator draft  does not matches with the visual drafts, until certain weights are added in ship store section ( In ballast- 3330 MT, In loaded- 4520 MT). The visual & loadicator drafts compared during loading at Salina Cruz, Mexico. Above observation found to be right, as weights are to be added to match the drafts. \nNew Loadicator computer / hardware ordered vide reqn no. DPEO245082.\n\nReceived new loadicator PC & installation completed. Will compare visual draft with loadicator at next available opportunity.","2025-05-30T08:00:00","DPEO245082","In progress",null,"No","No","Yes","Internal"]
[null,null,null,null,32530,"50_Tue Mar 26 2024 17:24:08 GMT+0800","2024-07-11T08:00:00","Defect","Ship Staff","Ship Staff Insp.","1.\t2 Stbd Cot valve indication not operational","","Cargo / Ballast Systems","Equipment Related","","","","","Troubleshooting carried out and found that the zener barrier is faulty and requires renewal. RO DPEO250065 placed for the same.. ","2025-05-15T08:00:00","DPEO250065","Waiting spare",null,"No","No","No","Internal"]
[null,null,null,null,19798,"50_Thu Dec 26 2024 23:28:47 GMT+0800","2024-12-12T08:00:00","Observation","Ship Staff","Ship Staff Insp.","PV valves are leaking slightly from the pressure side","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.19","High","","","Onboard spares consumed, DPEO250029 raised, pls arrange to supply around 02  Mar 2025.\nPV spares received. Renewal of spares in progress. ETC -30 APR 2025.\nAll PV valve purge pipe O-rings renewed. Leaking PV valve overhauled. Vessel intend to carry to vapor test of all PV valves. - ETC - 05 May 2025","2025-05-15T08:00:00","","In progress",null,"No","No","No","Internal"]
[null,null,null,null,33522,"50_Mon Feb 24 2025 17:11:25 GMT+0800","2025-02-23T08:00:00","Observation","Ship Staff","Ship Staff Insp.","OWS,Consumable filters is consumed and require one set a spares ","E/R - Purifier,Critical Equip.","Eng. / Strg. Comp.","Equipment Related,Inappropriate Procedure","10.32","Very High","","","RO has been raised for spares.(Critical spares ROB)","2025-05-23T08:00:00","DPEO250128","Waiting spare",null,"No","No","No","Internal"]
[null,null,null,null,58758,"50_Mon Feb 24 2025 21:51:49 GMT+0800","2025-02-02T08:00:00","Observation,Defect","Ship Staff","Ship Staff Insp.","Refer Provision compressor unit malfunctioning for PCB Control.","Elect. Mach. & Equip.","MLC Related","Equipment Related,External Factors,Human Error","10.32","Very High","","","Complete controller PCB unit to be renewed.","2025-05-20T08:00:00","DPEO250104","Waiting spare",null,"No","No","No","Internal"]
[null,null,null,null,33850,"50_Mon Feb 24 2025 21:53:24 GMT+0800","2025-02-03T08:00:00","Defect,Observation","Ship Staff","Ship Staff Insp.","Main engine Water in Oil sensor unit sensor is malfunctioning","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related,External Factors,Inappropriate Procedure","10.32","Very High","","","Sensor unit to be renewed.","2025-05-20T08:00:00","DPEO250103","Waiting spare",null,"No","No","No","Internal"]
[null,null,null,null,73171,"50_Mon Jan 13 2025 15:20:09 GMT+0800","2025-01-13T08:00:00","Defect,Observation","Ship Staff","Ship Staff Insp.","IG Scrubber inlet cone from uptake boiler need to be checked for leakages.","Cargo Mach.,E/R - Pipes/ valves & fittings","Cargo / Ballast Systems","Equipment Related,External Factors,Inappropriate Procedure","10.32","Very High","","","Cone section & inlet bellow to be checked for any sign of water or gas leakages from bellow or from flanges or any sign of crack in the pipelines. Will check and opportunity.","2025-05-30T08:00:00","","In progress",null,"No","No","No","Internal","Send a separate mail with pictures. Is there any part number for this Cone to order new?"]
[null,null,null,null,19574,"50_Tue Apr 22 2025 17:11:55 GMT+0800","2025-03-21T08:00:00","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","All damaged weather tight doors rain protector coaming to carry out soft repair. For permanent repair, add the job in REFMAN","Accommodation","Structural Condn. / WT integrity ","Equipment Related","","","","","All weather tight doors rain protectors coaming soft repair carried out. Job will be added in ref man","2025-05-30T08:00:00","","In progress",null,"No","No","No","Internal"]
[null,null,null,null,95346,"50_Wed Apr 30 2025 04:31:27 GMT+0800","2025-04-12T08:00:00","Observation","Ship Staff","Ship Staff Insp.","Stbd M/E RPM indicator showing less RPM by 6","Navigation - Others","Navigation","Equipment Related","","","","","Work in progress with Shore advice recvd on email.","2025-05-30T08:00:00","","In progress",null,"No","No","No","Internal"]

{"sheet":"Completed","index":1,"n_rows":1113,"n_cols":28,"rows_kept":1113,"cut":false,"hidden":false,"merged":[[10,8,10,9],[10,12,10,13],[12,6,12,27],[8,6,8,27]]}
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,"Defect - Damage Monitoring Sheet"]
[]
[null,null,null,null,null,null,null,"Date of Report","30-Apr-2025",null,null,"Ship Name","DHT PEONY (17-02-2025)"]
[]
[null,null,null,null,null,null,"VERSION : 2.0"]
[]
[]
[]
[null,null,null,"ID","SHIPSIDE UNIQUEID","UNIQUE ID","Date Recorded","Type of Deficiency","Observer code","Type of Inspection","Description of Deficiency","Equipment Categories","Area of Observation","Deficiency Cause","VIQ Ref Number","Risk Value of Obs","PSC Ref Number","PSC MOU ID","Action Taken or Required","Target Date","PO Ref No.","Status Code","Date Completed","Drydock","Info Sharing","Critical Item","Audit Type","Superintendent Remarks"]
[null,null,null,33811,92963,"50_Sat Feb 03 2024 06:26:13 GMT+0800",null,"Defect","Ship Staff","Ship Staff Insp.","EGCS WMS 002 unit sample pump not developing pressure","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Ship staff opened up the wms # 2 sampling pump, found inside rubber impeller was moving on the fixed nut and shaft key and key slot was worn out.The pump and motor assembly renewed with a new spare.","2024-03-31T23:59:35","","Completed","2024-02-15T23:59:35","No","No","No","Internal"]
[null,null,null,4087,null,"50_24/10/2019 3:58:30 PM","2019-01-26T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Pump room overboard ballast line leaking from the flange","Deck - Pipe / Fittings","Cargo / Ballast Systems","Behaviour Based,Equipment Related","8.8","Medium","","","Gasket to be changed during dry dock","2019-10-22T23:59:35","","Completed","2019-10-21T23:59:35","Yes","No","No","Internal"]
[null,null,null,4088,null,"50_24/10/2019 4:20:44 PM","2019-04-07T23:59:35","Defect","Ship Staff","Ship Staff Insp.","DRAFT GAUGE LINE IN 3P WBT HAVE PINHOLE LEAKAGE","Hull & Tanks","Cargo / Ballast Systems","Equipment Related","8.8","Medium","","","COLD REPAIRS DONE, SECTIONS RENEWED IN DRY DOCK","2019-06-25T23:59:35","","Completed","2019-10-21T23:59:35","No","No","No","Internal"]
[null,null,null,4089,null,"50_24/10/2019 4:23:40 PM","2019-04-07T23:59:35","Defect","Ship Staff","Ship Staff Insp.","GAS SAMPLING LINE FOR 3S WBT FWD POINT FOUND FULLY BLOCKED WITH METALLIC OBSTRUCTION IN CENTRELINE BULKHEAD AREA (PASSING FROM 3P TO 3S IN DB)","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","5.21","Medium","","","Line was found to be choked near bulkhead penetration. Same has been cleared during routine tank inspection carried out on 4th April 2020","2021-04-23T23:59:35","","Completed","2020-03-30T23:59:35","Yes","No","No","Internal"]
[null,null,null,4090,null,"50_24/10/2019 4:26:05 PM","2019-04-10T23:59:35","Defect","Ship Staff","Ship Staff Insp.","TG VACUUM CONDENSER SEA WATER INLET VALVE LEAKING FROM BODY.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","TEMPORARY REPAIRS CARRIED OUT/ VALVE RENEWED AFTER RECEIVING SAME.","2019-09-25T23:59:35","DPOE190052","Completed","2019-06-01T23:59:35","No","No","No","Internal"]
[null,null,null,4091,null,"50_24/10/2019 4:28:48 PM","2019-04-10T23:59:35","Defect","Ship Staff","Ship Staff Insp.","ME STARTING AIR PRESSURE ON BRIDGE CONSOLE INCORRECT READING, SHOWS 11 BAR LESS THAN ACTUAL","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","SPARES  RECEIVED  ON 25/05/19","2020-01-10T23:59:35","DPEO190028//RECEIVED ALREADY ON 25/05/19","Completed","2019-05-20T23:59:35","No","No","No","Internal"]
[null,null,null,4106,null,"50_24/10/2019 4:31:30 PM","2019-05-10T23:59:35","Defect","Ship Staff","Ship Staff Insp.","IG BRANCH VALVE FOR 1C,2C,3C,4C,5C,5S,SLOP P&S FOUND LEAKING","Inert Gas","Cargo / Ballast Systems","Equipment Related","8.2","Medium","","","ALL VALVES SEAT RINGS RENEWED","2019-07-25T23:59:35","","Completed","2019-08-23T23:59:35","No","No","No","Internal"]
[null,null,null,8079,null,"50_16/12/2019 11:35:12 AM","2019-05-12T23:59:35","Defect","FSC Inspector","Flag State Insp.","Original contract letters of Fitter, Cook, AB and newly promoted AB was not on board and only scanned copies was on board","Documentation","Crew Management","Inappropriate Procedure","3.1","High","","","Original congtract received from manning office","2019-05-20T23:59:35","","Completed","2019-06-22T23:59:35","No","No","No","External"]
[null,null,null,4096,null,"50_24/10/2019 4:44:59 PM","2019-05-13T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","LO PURIFIER #2 STEAM REGULATING VALVE MECHANISM BROKEN AND NOT OPERATIONAL","E/R - Aux. Mach.,E/R - Purifier","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","REQUISITION RAISED//RECEIVED,FITTED STILL NOT RERSPONDING, CONVERSATION WITH MAKER ON","2020-01-25T23:59:35","DPEO190154// RECEIVED IN SHIPYARD","Completed","2019-10-18T23:59:35","No","No","No","Internal"]
[null,null,null,4101,null,"50_24/10/2019 4:47:34 PM","2019-05-13T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","FIRE HOSE BOX NEAR LIFEBOAT PORT & STBD FOUNDATION BROKEN\t","LSA / FFA","Eng. / Strg. Comp.","External Factors","5.38","High","","","FOUNDATION RENEWED IN DRYDOCK","2019-06-25T23:59:35","","Completed","2019-10-16T23:59:35","No","No","No","Internal"]
[null,null,null,4102,null,"50_24/10/2019 4:57:36 PM","2019-05-13T23:59:35","Defect","Ship Staff","Ship Staff Insp.","2C MAIN VALVE LEAKING CARGO\t\t","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.11","Medium","","","SEAT RING RENEWED DURING TANK INSPECTION","2019-08-13T23:59:35","","Completed","2019-09-24T23:59:35","No","No","No","Internal"]
[null,null,null,4103,null,"50_24/10/2019 4:55:14 PM","2019-05-13T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","3S MAIN VALVE SUSPECT LEAKING","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.11","Medium","","","CHECKED DURING COT INSPECTION , NOT LEAKAGE FOUND","2019-08-13T23:59:35","","Completed","2019-09-24T23:59:35","No","No","No","Internal"]
[null,null,null,4086,null,"50_24/10/2019 4:52:58 PM","2019-05-13T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","GALLEY DISH WASHER NOT OPERATIONAL","Miscellaneous","General Appearance","Equipment Related","11.16","Low","","","DRAIN TO BE CLEARED IN DD","2019-07-10T23:59:35","","Completed","2019-10-24T23:59:35","No","No","No","Internal"]
[null,null,null,4092,null,"50_24/10/2019 4:33:59 PM","2019-05-13T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Ship Staff Insp.","STROP COUPLING ON ME SCAVANGE RECEIVER DRAIN LINES LEAKING","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","REQUISITION RAISED/ RECEIVED ON 01/10/19 IN DRY DOCK. 7 PIECES RENEWED.","2020-01-11T23:59:35","DPEO190157 // RECEIVED 01/10/19","Completed","2019-12-20T23:59:35","No","No","No","Internal"]
[null,null,null,4093,null,"50_24/10/2019 4:36:27 PM","2019-05-13T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ME NO.1 FUEL PUMP BLOCK SLIGHTLY LEAKING FROM VALVE TOP COVERS","Deck - Machinery,E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","JOB INCLUDED IN REFMAN/// COMPLETED IN DRYDOCK BY SHORE WORKSHOP","2019-10-25T23:59:35","","Completed","2019-10-20T23:59:35","No","No","No","Internal"]
[null,null,null,4094,null,"50_24/10/2019 4:37:55 PM","2019-05-13T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","EGB CLADDING DAMAGED AND TO BE RENEWED","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","JOB INCLUDED IN REFMAN// COMPLETED IN DRYDOCK BY SHORE","2019-08-11T23:59:35","","Completed","2019-10-24T23:59:35","No","No","No","Internal"]
[null,null,null,4095,null,"50_24/10/2019 4:42:44 PM","2019-05-13T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","LO PURIFIER# 1 STEAM REGULATING VALVE MECHANISM BROKEN AND NOT OPERATIONAL","E/R - Boiler,E/R - Purifier","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","REQUISISTION RAISED// RECEIVED,FITTED STILL NOT RERSPONDING, CONVERSATION WITH MAKER ON","2020-01-25T23:59:35","DPEO190154// RECEIVED IN SHIPYARD","Completed","2019-10-18T23:59:35","No","No","No","Internal"]
[null,null,null,4097,null,"50_24/10/2019 5:00:07 PM","2019-05-21T23:59:35","Defect","Ship Staff","Ship Staff Insp.","AUX BOILER #2 CHEMICAL DOSING PUMP NOT OPERATIONAL","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","AWAITING SPARES// received, pump renewed","2019-08-15T23:59:35","DPEO190044// received","Completed","2019-11-09T23:59:35","No","No","No","Internal"]
[null,null,null,4098,null,"50_24/10/2019 5:01:43 PM","2019-05-21T23:59:35","Defect","Ship Staff","Ship Staff Insp.","BOILER LOCAL AND MAIN CONTROL PANEL WINDOW AC  NON OPERATIONAL","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","AWAITING SPARES-NA. REPAIRED IN SHIPYARD. AGAIN LOCAL PANEL AC NOT WORKING.","2020-01-15T23:59:35","DPEO190046// RO CANCELLED BY OFFICE","Completed","2019-10-18T23:59:35","No","No","No","Internal"]
[null,null,null,8080,null,"50_16/12/2019 11:37:47 AM","2019-05-21T23:59:35","Non Conformity","Owner / Marine / Tech. Suptd.","ISM Audit","LSA Training manual data not ship specific : Location / Quantity of equipment , Procedure to use the recovery strops/ recover Rescue boat in rough weather missing","LSA / FFA","Safety / LSA / FFA","Human Error","5.27","Medium","","","The Safety and Training manual to be reviewed on a regular basis the by responsible officer","2019-08-21T23:59:35","","Completed","2019-06-10T23:59:35","No","No","No","Internal"]
[null,null,null,8081,null,"50_16/12/2019 11:39:14 AM","2019-05-21T23:59:35","Defect","Owner / Marine / Tech. Suptd.","ISM Audit","Some of the isolation valves in foam room are not marked ","LSA / FFA","Safety / LSA / FFA","Human Error","5.4","High","","","The officer and crew were reminded that after any cosmetic maintenance, the markings for identification should be done immediately.\n\nThe safety officer should verify this during his safety rounds.","2019-08-21T23:59:35","","Completed","2019-06-10T23:59:35","No","No","No","Internal"]
[null,null,null,8082,null,"50_16/12/2019 11:41:27 AM","2019-05-21T23:59:35","Defect","Owner / Marine / Tech. Suptd.","ISM Audit","Placard for Garbage in accordance to MARPOL Annex V not available at the Garbage collection/ Handling area ","Documentation","MARPOL Related","Human Error","6.2","High","","","The placards were posted in the required locations.","2019-08-21T23:59:35","","Completed","2019-06-10T23:59:35","No","No","No","Internal"]
[null,null,null,8083,null,"50_16/12/2019 11:43:11 AM","2019-05-21T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Mooring Audit","MBL marking not present on the mooring winches (Refer Mooring Equipment Guidelines 4)","Deck - Mooring Machinery","Mooring","Human Error","9.19","Low","","","Marking were done on the mooring winches","2019-08-21T23:59:35","","Completed","2019-06-10T23:59:35","No","No","No","Internal"]
[null,null,null,8084,null,"50_16/12/2019 11:44:58 AM","2019-05-21T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Nav Audit / Verification","Security levels were not indicated for all legs of the voyage","Navigation - Others","Navigation","Human Error","7.4","Low","","","The security level included for each leg","2019-08-21T23:59:35","","Completed","2019-06-10T23:59:35","No","No","No","Internal"]
[null,null,null,8085,null,"50_16/12/2019 11:47:11 AM","2019-05-21T23:59:35","Defect","Owner / Marine / Tech. Suptd.","ISM Audit","The log of inspection of lifting equipment in engine room was not upto date. Some of the new chain blocks were not included in the list.","Documentation","Eng. / Strg. Comp.","Human Error","8.5","Very High","","","The list was updated with the new chain blocks also.","2019-08-21T23:59:35","","Completed","2019-06-10T23:59:35","No","No","No","Internal"]
[null,null,null,4099,null,"50_24/10/2019 5:04:39 PM","2019-06-05T23:59:35","Defect","Ship Staff","Ship Staff Insp.","PAINT STORE AND PUMP ROOM STBD SIDE DOOR CHANNEL FOUND IN CORRODED CONDITION","Miscellaneous","Structural Condn. / WT integrity ","Equipment Related","11.6","Medium","","","TO BUILD UP THE HOLES- DOOR REPAIRED AND REFITTED.","2020-03-25T23:59:35","","Completed","2020-01-09T23:59:35","No","No","No","Internal"]
[null,null,null,4100,null,"50_24/10/2019 5:11:40 PM","2019-06-11T23:59:35","Defect","Ship Staff","Ship Staff Insp.","ACCESS HATCH FOR MAST RISER PLATFORM BROKEN FROM HINGES, CHECKERED PLATE THINNED DOWN","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","External Factors","11.5","Medium","","","CHECKERED PLATE CROPPED, NEW PLATE TO BE WELDED AND NEW DOOR TO BE FABRICATED TO BE FITTED","2020-03-25T23:59:35","","Completed","2019-12-28T23:59:35","No","No","No","Internal"]
[null,null,null,4105,null,"50_24/10/2019 5:14:06 PM","2019-06-11T23:59:35","Defect","Ship Staff","Ship Staff Insp.","MAIN MAST PLATFORM ACCESS DOOR HINGES BADLY CORRODED, DOOR UNABLE TO MOVE","Accommodation","General Appearance","External Factors","11.5","Medium","","","DOOR CROPPED AND NEW DOOR FITTED","2019-09-25T23:59:35","","Completed","2019-10-15T23:59:35","No","No","No","Internal"]
[null,null,null,4104,null,"50_24/10/2019 5:18:32 PM","2019-08-15T23:59:35","Defect","Ship Staff","Ship Staff Insp.","BALLAST EDUCTOR SUCTION VALVE BEV 64 SUSPECT LEAKING, TO BE RECTIFIED IN DD","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.11","Medium","","","BEV 64 OPENED FOUND PIECE OF RUBBER STUCK AROUND SEAT, SAME REMOVED.SEAT RING FOUND OK","2019-10-10T23:59:35","","Completed","2019-10-17T23:59:35","No","No","No","Internal"]
[null,null,null,8086,null,"50_16/12/2019 11:58:51 AM","2019-09-09T23:59:35","Defect","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","It was observed that several securing screws/bolts were missing from\n\nthe floor plates located in purifier room.","Elect. Mach. & Equip.,E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Human Error","10.29","Medium","","","Missing floor plates screws and bolts fixed","2019-12-09T23:59:35","","Completed","2019-09-09T23:59:35","No","No","No","External"]
[null,null,null,8087,null,"50_16/12/2019 12:02:47 PM","2019-09-09T23:59:35","Defect","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","The paint on midships draft marks, as seen on port side, was noted to\n\nbe faded/removed.\n\nAs per annual survey report issued by Class ABS dated 01 Feb 2019, an outstanding additional\n\nrequirement (No. 32), originally issued in Jan 2018, stated that the 'Loadline marks of the\n\nprevious assigning authority/society in way of the rings are to be grounded off and the 'AB'\n\nmarks are to be permanently marked (punched, welded or raised letters welded to the side\n\nshell) and painted'. Due date: 28 Apr 2021.","Hull & Tanks","Structural Condn. / WT integrity ","Industry Issue","11.2","Medium","","","Completed in dry dock","2021-04-23T23:59:35","","Completed","2019-10-24T23:59:35","No","No","No","External"]
[null,null,null,8088,null,"50_16/12/2019 12:06:48 PM","2019-09-09T23:59:35","Defect","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","The airline section, located near the cargo pump room and connected\n\nto port side pneumatic actuator to operate cargo pump room's vent flap, had been temporarilyrepaired by bandage/putty (length of temporary repair was around 150 mm - pipe size 15A).","Cargo Mach.","Structural Condn. / WT integrity ","Inappropriate Procedure","11.4","Very High","","","New pipe raangement fabricated","2019-12-09T23:59:35","","Completed","2019-10-24T23:59:35","No","No","No","External"]
[null,null,null,9053,null,"50_25/12/2019 3:45:12 PM","2019-11-16T23:59:35","Defect","Ship Staff","Nav Audit / Verification","Some of the entries in deck log book were missing as per the entries to be made bell book/deck log book","Navigation - Others","Navigation","Human Error","4.2","Medium","","","Entries were immediately corrected post audit","2019-12-16T23:59:35","","Completed","2019-11-18T23:59:35","No","No","No","Internal"]
[null,null,null,9605,null,"50_14/01/2020 7:06:42 PM","2019-12-05T23:59:35","Defect","FSC Inspector","OM Insp. (Eg. SIRE / CDI etc.)","LOW INSULATION ON MSB","Elect. Mach. & Equip.","Eng. / Strg. Comp.","External Factors","10.38","Medium","","","INVESTIGATED AND FOUND ONE LIGHT SWITCH ON BRIDGE WINGS WITH MOISTURE FOLLOWING HEAVY RAINS.SAME DISMANTLED AND SERVICED","2020-01-20T23:59:35","","Completed","2019-12-06T23:59:35","No","No","No","External"]
[null,null,null,8078,null,"50_13/12/2019 11:56:45 AM","2019-12-05T23:59:35","Defect","Ship Staff","Ship Staff Insp.","IG SCRUBBER DISCHARGE PIPE HOLED IN MULTIPLE PLACES","Inert Gas","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","NO SPARE PIPE ONBOARD, SAME REQUISITIONED and RECEIVED . WILL RENEW IN VOYAGE, ONE LENGTH FABRICATED. BOTH LENGTHS FABRICATED AND FITTED","2020-01-26T23:59:35","DPEO 190265- ALREADY RECEIVED","Completed","2019-12-30T23:59:35","No","No","No","Internal"]
[null,null,null,8089,null,"50_16/12/2019 12:12:03 PM","2019-12-05T23:59:35","Defect","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","Main switch board was noted with an earth alarm on 220 volt panel","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Human Error","10.38","Medium","","","Rectified during inspection.Rectiied during inspection","2019-12-05T23:59:35","","Completed","2019-12-05T23:59:35","No","No","No","External"]
[null,null,null,8090,null,"50_16/12/2019 12:15:44 PM","2019-12-05T23:59:35","Defect","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","The loadlines marked on the vessel refelected a summer deadweight of 299999 MT ( second deepest).The active loadline as per class records was 320013 MT","Hull & Tanks","Structural Condn. / WT integrity ","Knowledge Based","11.2","Medium","","","After further inspection , the correct load lines are found marked on ship side  as per active DWT 299999 MT as per class records ","2020-03-05T23:59:35","","Completed","2020-03-15T23:59:35","No","No","No","External"]
[null,null,null,9604,null,"50_14/01/2020 9:15:43 AM","2020-01-01T23:59:35","Observation","Owner / Marine / Tech. Suptd.,Ship Staff","Suptd. Insp.","CAPACITORS IN FLOURESCENT TO LED LIGHT FITTING CONVERSION IN ACCCOMODATION TO BE DISCONNECTED FROM THE CIRCUIT DURING CONVERSION","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","11.16","Low","","","BEING DONE UPON ANY FITTING CONVERSION ALL FITTINGS IN ACCOMODATION CHECKED. ALL CAPACITORS CONFIRMED DISCONNECTED FOR ALL FLOURESCENT FITTINGS THAT HAVE BEEN REPLACED WITH LED LAMPS","2020-06-30T23:59:35","","Completed","2020-01-23T23:59:35","No","No","No","Internal"]
[null,null,null,10569,null,"50_01/02/2020 11:12:56 AM","2020-01-25T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Wheelhouse Defrosting Heater coil giving 440V low insulation alarm","Navigation - Others","Navigation","Equipment Related","4.7","High","","","New heater coil recvd at singapore. Heater coil fitted and equipment tried out. Working satisfactory","2020-07-25T23:59:35","","Completed","2020-05-13T23:59:35","No","No","No","Internal"]
[null,null,null,11898,null,"50_03/04/2020 7:23:30 AM","2020-01-27T23:59:35","Defect","Ship Staff","Ship Staff Insp.","BEV65 ballast eductor suction valve body cracked and leaking","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.11","Medium","","","valve renewed and tried out . Working satisfactory","2020-04-29T23:59:35","DPEO200075","Completed","2020-06-05T23:59:35","No","No","No","Internal",""]
[null,null,null,10570,null,"50_18/02/2020 4:33:28 AM","2020-02-04T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","5P PV Valve mesh corroded and other PV Valve mesh having salt deposits","Inert Gas","Cargo / Ballast Systems","External Factors","8.19","High","","","5P mesh renewed and rest all PV valve mesh cleaned.","2020-05-04T23:59:35","","Completed","2020-02-16T23:59:35","No","No","No","Internal"]
[null,null,null,10571,null,"50_18/02/2020 4:42:41 AM","2020-02-04T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Port and Stbd Anchor wash leaking from the Valve glands.","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.4","Very High","","","Both anchor wash overhauled","2020-05-04T23:59:35","","Completed","2020-02-27T23:59:35","No","No","No","Internal"]
[null,null,null,10572,null,"50_18/02/2020 4:51:17 AM","2020-02-04T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Slop heating coils and COW Branch lines to be De-rusted, buffed and painted","Deck - Pipe / Fittings","General Appearance","Equipment Related","8.15","High","","","Slop heating coils buffed and painted ","2020-05-04T23:59:35","","Completed","2020-02-24T23:59:35","No","No","No","Internal"]
[null,null,null,10573,null,"50_18/02/2020 4:45:24 AM","2020-02-04T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Vapor manifold drains do not have caps at the end.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","6.8","High","","","Caps for Vapour manifold Drain pipes - Fabricated and fitted in place","2020-05-04T23:59:35","","Completed","2020-08-14T23:59:35","No","No","No","Internal","Pls land sample at Singapore for fabrication - and update the status of the landed date in DDRL"]
[null,null,null,10574,null,"50_21/02/2020 3:17:16 AM","2020-02-04T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Main Engine Shaft Power Meter not working","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Lemag shaft power sensors received. Sensor renewed.","2020-07-27T23:59:35","DPEO190230","Completed","2020-06-24T23:59:35","No","No","No","Internal"]
[null,null,null,10575,null,"50_18/02/2020 4:29:41 AM","2020-02-04T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Liferaft launching instruction on Port and Stbd accomodation block not fully specific to actual arrangement","LSA / FFA","Safety / LSA / FFA","Behaviour Based,Human Error","5.15","Medium","","","Ship specific life raft launching procedure made and displayed underneath emergency light near liferaft launching station","2020-05-04T23:59:35","","Completed","2020-02-14T23:59:35","No","No","No","Internal"]
[null,null,null,10576,null,"50_18/02/2020 4:11:34 AM","2020-02-04T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Stbd aft vapor manifold drain valve not holding and leaking","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.42","Medium","","","New drain pipe fabricated by hotwork on poop deck.","2020-05-04T23:59:35","","Completed","2020-02-09T23:59:35","No","No","No","Internal"]
[null,null,null,10577,null,"50_18/02/2020 4:21:25 AM","2020-02-04T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","2P and 4S PV Valve vacuum side leaking heavily and other PV Valves need to be checked for Vapour tightness","Inert Gas","Cargo / Ballast Systems","Equipment Related","8.19","High","","","2P and 4S PV valve overhauled.Leak checks carried out for all PV.No leaks observed","2020-05-04T23:59:35","","Completed","2020-02-10T23:59:35","No","No","No","Internal"]
[null,null,null,10578,null,"50_18/02/2020 4:25:13 AM","2020-02-04T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","X Band radar not displaying targets","Navigation - RADAR","Navigation","Equipment Related","4.7","High","","","Magnetron replaced and wave guide air blown.X band radar operational.","2020-05-04T23:59:35","","Completed","2020-02-06T23:59:35","No","No","No","Internal"]
[null,null,null,10579,null,"50_18/02/2020 4:49:01 AM","2020-02-04T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Poop deck stbd Mooring winch platform guard dislodged","Deck - Mooring Machinery","Mooring","Human Error","9.14","Medium","","","Platform fixed back by hotwork on poop deck","2020-05-04T23:59:35","","Completed","2020-02-08T23:59:35","No","No","No","Internal"]
[null,null,null,10580,null,"50_18/02/2020 6:18:25 AM","2020-02-04T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Nav Audit / Verification","SAFETY CONTOUR AND SAFTEY DEPTH VALUES WRONGLY CALCULATED IN PASSAGE PLAN FROM JUAYMAH TO PAL.","Navigation - ECDIS","Navigation","Human Error","4.5","Very High","","","SAFETY CONTOUR AND SAFTEY DEPTH VALUES WERE CORRECTED AS PER UKC POLICY","2020-05-03T23:59:35","","Completed","2020-02-05T23:59:35","No","No","No","Internal"]
[null,null,null,10581,null,"50_18/02/2020 6:22:02 AM","2020-02-04T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Nav Audit / Verification","SIMILIAR ENGINE SPEED FOR AHEAD AND ASTERN IS MENTIONED IN THE PILOT CARD","Navigation - Others","Navigation","Human Error","4.3","Medium","","","PILOT CARD WAS CORRECTED FOR ENGINE SPEEDS, AHEAD AND ASTERN VALUES.","2020-05-03T23:59:35","","Completed","2020-02-05T23:59:35","No","No","No","Internal"]
[null,null,null,10582,null,"50_18/02/2020 6:26:34 AM","2020-02-04T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Nav Audit / Verification","BRIDGE COMPUTERS NOT HAVING THE FOLLOWING WARNING POSTERS \" TO USED ONLY FOR WATCH RELATED/NAVIGATION PURPOSES BY WATCHKEEPERS\"","Miscellaneous","Navigation","Inappropriate Procedure","4.1","High","","","WARNING POSTER \" TO USED ONLY FOR WATCH RELATED/NAVIGATION PURPOSES BY WATCHKEEPERS\" WERE POSTED ON BRIDGE COMPUTERS.","2020-05-03T23:59:35","","Completed","2020-02-05T23:59:35","No","No","No","Internal"]
[null,null,null,10583,null,"50_18/02/2020 6:40:38 AM","2020-02-04T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","BEST MANAGEMENT PRACTICE POSTER OF \"SWITCH OFF LIGHTS WHEN NOT IN USE\" NOT POSTED IN COMMON SPACES OF ACCOMODATION.","Accommodation","MARPOL Related","Inappropriate Procedure","2.14","Low","","","BEST MANAGEMENT PRACTICE POSTER OF \"SWITCH OFF LIGHTS WHEN NOT IN USE\" POSTED IN COMMON SPACES OF ACCOMODATION.","2020-05-03T23:59:35","","Completed","2020-02-07T23:59:35","No","No","No","Internal"]
[null,null,null,10584,null,"50_18/02/2020 6:30:53 AM","2020-02-04T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Nav Audit / Verification","MASTER'S NIGHT ORDERS FROM 10TH JAN 2020 TO 31ST JAN 2020 HAVE BEEN WRITTEN FOR 2 DAYS ON A SINGLE PAGE WITH ONLY ONE ACKNOWLEDGEMENT SIGNATURE BY WATCHKEEPERS AT THE END OF THE PAGE.","Miscellaneous","Navigation","Human Error","4.2","Medium","","","WATCHKEEPERS SIGNED NIGHT ORDERS FOR EACH DAY IRRESPECTIVE OF THE PAGE.","2020-05-03T23:59:35","","Completed","2020-02-05T23:59:35","No","No","No","Internal"]
[null,null,null,10639,null,"50_21/02/2020 9:22:10 AM","2020-02-15T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","2C TGE unit failure","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.19","High","","","2C TGE unit to be replaced","2020-05-15T23:59:35","DPEO200032","Completed","2020-04-29T23:59:35","No","No","No","Internal"]
[null,null,null,10640,null,"50_28/02/2020 8:30:46 PM","2020-02-15T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","H2S sensor for fixed gas detetion system in pumproom failure","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.46","Very High","","","H2S sensor in Pump room has been replaced with new sensor received in Last call Singapore . Working satisfactory ","2020-05-15T23:59:35","DPEO200035","Completed","2020-07-14T23:59:35","No","No","No","Internal"]
[null,null,null,10638,null,"50_28/02/2020 8:36:34 PM","2020-02-23T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Cargo Audit","Vessel on loaded condition but Pre arrival checks recorded in CCR log on 4th Feb 2020 indicates surface of all WBT`s checked for oil sheen and samples drawn. Pre arrival checks section D item number 15 answered as NA.","Documentation","Cert. & Docu.","Human Error","2.16","Medium","","","Same corrected in checklist and CCR log","2020-05-23T23:59:35","","Completed","2020-02-25T23:59:35","No","No","No","Internal"]
[null,null,null,10641,null,"50_28/02/2020 8:37:51 PM","2020-02-23T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Cargo Audit","Evidence not provided to show that the valve line up was cross checked by two officers. CCR log indicates line up for discharging and venting individually checked by 3 off. ","Documentation","Cargo / Ballast Systems","Human Error","8.5","Very High","","","Same corrected and logged","2020-05-23T23:59:35","","Completed","2020-02-25T23:59:35","No","No","No","Internal"]
[null,null,null,10642,null,"50_28/02/2020 8:39:23 PM","2020-02-23T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Cargo Audit","No evidence to show that entries were made as per 12.21.03.001.00 prior to use of vapour emission control system (oil)","Documentation","Cargo / Ballast Systems","Human Error","8.5","Very High","","","Same logged in CCR log in pre arrival checks","2020-05-23T23:59:35","","Completed","2020-02-25T23:59:35","No","No","No","Internal"]
[null,null,null,10643,null,"50_28/02/2020 8:40:46 PM","2020-02-23T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Cargo Audit","Pre arrival check list was completed after the vessel commenced discharge operation.(07 Feb 2020)  ","Documentation","Cargo / Ballast Systems","Human Error","8.5","Very High","","","corrected for the same ","2020-05-23T23:59:35","","Completed","2020-02-25T23:59:35","No","No","No","Internal"]
[null,null,null,10644,null,"50_29/02/2020 6:17:45 AM","2020-02-23T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Engineering Audit","Serial Number of Purifier and Safety routines (Job Order) of purifiers to be added in PAL PMS","Documentation,E/R - Purifier","Cert. & Docu.","Equipment Related","10.12","Very High","","","CRF FILLED AND SENT TO OFFICE FOR CORRECTION","2020-07-27T23:59:35","","Completed","2020-05-09T23:59:35","No","No","No","Internal"]
[null,null,null,10645,null,"50_28/02/2020 8:42:20 PM","2020-02-23T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Bunkering Audit","Bunkering safety check list 12.04.08.014.00 code A is not signed by both parties.  ","Documentation","Cert. & Docu.","Human Error","10.8","Medium","","","Tick marks were initially placed to record agreement and common signature placed for the column. Now individual places specifiing A have been signed by vessel","2020-05-23T23:59:35","","Completed","2020-02-23T23:59:35","No","No","No","Internal"]
[null,null,null,18646,null,"50_19/03/2021 09:55:17","2020-03-08T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Oil leakages on steering gear system","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Both S/G system pumps and hydraulic blocks overhaued in 2021 dry dock. Pump mech seals and other seal renewed. No leakage obsrved after system put in to use.","2020-06-08T23:59:35","","Completed","2021-02-26T23:59:35","No","No","No","Internal"]
[null,null,null,11107,null,"50_01/04/2020 2:20:17 AM","2020-03-25T23:59:35","Defect,Observation","Owner / Marine / Tech. Suptd.","Ship Staff Insp.","MS Bolts of hose handling crane working platform to renewed with Stainless steel SUS 316 bolts","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","Equipment Related","8.5","Very High","","","existing bolts were removed from location and checked and were found to be SS . No need for renewal .","2020-06-25T23:59:35","","Completed","2020-05-20T23:59:35","No","No","No","Internal"]
[null,null,null,17499,null,"50_17/01/2021 07:37:00","2020-04-25T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","D/G #1 FO line flange leaking and portable container kept to collet leaking oil","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Section of pipes removed gaskets renewed.","2020-05-25T23:59:35","","Completed","2020-05-05T23:59:35","No","No","No","External"]
[null,null,null,17500,null,"50_17/01/2021 11:20:00","2020-04-25T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","EGB tube leaking","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Temporary repairs done. Renewal planed for DD. Root cause is excess pressure in line, need to fit a dump controller on the atmospheric condenser  line","2020-05-25T23:59:35","","Completed","2020-05-10T23:59:35","No","No","No","Internal"]
[null,null,null,17501,null,"50_18/01/2021 9:04:13 AM","2020-04-25T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","FO pipe leakage at atmosphere condenser deck","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Pipe gasket renewed.","2020-05-01T23:59:35","","Completed","2020-04-27T23:59:35","No","No","No","Internal"]
[null,null,null,17502,null,"50_18/01/2021 9:12:08 AM","2020-04-25T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","IG scrubber drain pipe flange has salt deposit and valve hand wheel missing","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Salts removed, valve handle seplaced with spare. ","2020-05-25T23:59:35","","Completed","2020-05-01T23:59:35","No","No","No","Internal"]
[null,null,null,17503,null,"50_18/01/2021 9:06:10 AM","2020-04-25T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","FO tank 1P valve gland leaking","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Gland tightened","2020-05-01T23:59:35","","Completed","2020-04-26T23:59:35","No","No","No","Internal"]
[null,null,null,17504,null,"50_18/01/2021 9:16:44 AM","2020-04-25T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Ship Staff Insp.","Main Engine air cooler (F) manometer dry","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Manometer filled up to the required level","2020-05-01T23:59:35","","Completed","2020-04-27T23:59:35","No","No","No","Internal"]
[null,null,null,17505,null,"50_18/01/2021 9:18:39 AM","2020-04-25T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Main Engine JCW pump (F) inlet pipe flange covered with salt","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Flange tightened. Salt removed","2020-05-01T23:59:35","","Completed","2020-04-29T23:59:35","No","No","No","Internal"]
[null,null,null,17506,null,"50_18/01/2021 9:26:46 AM","2020-04-25T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Main Engine under piston space temporary container","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Tightened bolts on the cover, leak arrested. container removed","2020-05-25T23:59:35","","Completed","2020-04-29T23:59:35","No","No","No","Internal"]
[null,null,null,17507,null,"50_18/01/2021 9:29:04 AM","2020-04-25T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Main Engine unit 1 and 2 fuel pump block leakage","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Fuel pump overhauled, leakage stopped","2020-07-25T23:59:35","","Completed","2020-10-10T23:59:35","No","No","No","Internal"]
[null,null,null,11108,null,"50_07/03/2020 1:05:05 AM","2020-04-25T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Hose handling crane (P) top hand rail corroded and broken","Deck - Machinery","Structural Condn. / WT integrity ","Equipment Related","8.5","Very High","","","Wasted sections renewed by hotwork with permission from office","2020-07-25T23:59:35","","Completed","2020-07-19T23:59:35","No","No","No","Internal","Pls include this in REFFMAN, if cannot be repaired and close the defect"]
[null,null,null,17508,null,"50_18/01/2021 9:38:00 AM","2020-04-25T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ME JCW condensate pipe sight glass to clean","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Sight glass cleaned. ","2020-05-01T23:59:35","","Completed","2020-05-01T23:59:35","No","No","No","Internal"]
[null,null,null,17509,null,"50_18/01/2021 9:42:50 AM","2020-04-25T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Oil leakage above ME JCW pump, on top of intermediate shaft bearing","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Flange on top of JCW pump ( incinerator waste oil tank drain line) tightened. no leaks at present.","2020-05-25T23:59:35","","Completed","2020-05-16T23:59:35","No","No","No","Internal"]
[null,null,null,17510,null,"50_18/01/2021 9:45:27 AM","2020-04-25T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Portable fire extinguisher in Engine room and SOx scrubber room not checked in April 2020","Miscellaneous","Eng. / Strg. Comp.","Human Error","5.42","Medium","","","Extinguisher inspected and signed.","2020-04-26T23:59:35","","Completed","2020-04-26T23:59:35","No","No","No","Internal"]
[null,null,null,17511,null,"50_18/01/2021 9:14:13 AM","2020-04-25T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","MAC (F) cooling water valve handle missing","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Valve handle replaced with spare","2020-05-02T23:59:35","","Completed","2020-04-30T23:59:35","No","No","No","Internal"]
[null,null,null,17512,null,"50_18/01/2021 9:47:13 AM","2020-04-25T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Insulation matt in front of Em. Fire pump start panel torn","Miscellaneous","Eng. / Strg. Comp.","Behaviour Based","10.24","Low","","","Insulation mat renewed","2020-05-25T23:59:35","","Completed","2020-04-26T23:59:35","No","No","No","Internal"]
[null,null,null,17513,null,"50_18/01/2021 9:49:10 AM","2020-04-25T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Insulation matt in front of soot blow panel and super heat stem panel missing","Miscellaneous","Eng. / Strg. Comp.","Human Error","10.24","Low","","","New mat put in place","2020-05-25T23:59:35","","Completed","2020-04-26T23:59:35","No","No","No","Internal"]
[null,null,null,17514,null,"50_18/01/2021 10:09:52 AM","2020-04-25T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Steering gear save all filled with oil","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Oil cleaned. valve blocks tightness checked. seals checked for leakages","2020-07-25T23:59:35","","Completed","2020-08-28T23:59:35","No","No","No","Internal"]
[null,null,null,17515,null,"50_18/01/2021 09:24:01","2020-04-25T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","PV breaker date for last clean & inspection not stenciled","Miscellaneous","Cargo / Ballast Systems","Human Error","8.28","Medium","","","Date stenciled","2020-05-01T23:59:35","","Completed","2020-04-27T23:59:35","No","No","No","Internal"]
[null,null,null,17516,null,"50_18/01/2021 9:52:18 AM","2020-04-25T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Vacuum condenser pump mechanical seal leaking","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Mech seal flange opened and repositioned the seal. no leak is visible at present.","2020-05-25T23:59:35","","Completed","2020-05-20T23:59:35","No","No","No","Internal"]
[null,null,null,11897,null,"50_15/05/2020 5:22:54 PM","2020-04-25T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","A deck common toilet door latch spoilt","Accommodation","MLC Related","Equipment Related","11.13","Low","","","To renew the lock ","2020-07-25T23:59:35","","Completed","2020-06-08T23:59:35","No","No","No","Internal"]
[null,null,null,11899,null,"50_08/05/2020 4:17:56 PM","2020-04-25T23:59:35","Defect,Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Exhasut gas was found leaking from AE#3 Exhasut pipe flange","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Staging made as leaking flange is at a height. Lagging removed and flange bolts to tighened after renewing the gasket","2020-05-23T23:59:35","","Completed","2020-05-15T23:59:35","No","No","No","Internal"]
[null,null,null,11900,null,"50_08/05/2020 4:23:19 PM","2020-04-25T23:59:35","Defect,Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Oil leaking from steering gear system","Critical Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Minor oil leakage from Ram end part rectified by replacing copper washer at the ram end screw.","2020-09-26T23:59:35","","Completed","2020-09-01T23:59:35","No","No","No","Internal"]
[null,null,null,11901,null,"50_15/05/2020 5:17:57 PM","2020-04-25T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Alleyway floor in front of Ship's Office damaged","Accommodation","General Appearance","Equipment Related","11.13","Low","","","Deferred to Dry dock as flooring needs to be rebuilt with new vinyl carpet.","2020-07-25T23:59:35","","Completed","2020-07-25T23:59:35","No","No","No","Internal"]
[null,null,null,11902,null,"50_15/05/2020 5:27:19 PM","2020-04-25T23:59:35","Defect,Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Cargo and Ballast system - Few valve position indicators in CCR not showing correct position of valves. Valve shut but showing open/ partial shut","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.8","Medium","","","Trouble shooting carried out and rectified valve position.","2020-07-25T23:59:35","","Completed","2020-07-19T23:59:35","No","No","No","Internal"]
[null,null,null,11903,null,"50_15/05/2020 5:31:08 PM","2020-04-25T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","COP Red and Yellow suction pressure gauge not showing zero when pump stopped","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.8","Medium","","","Pressure gauge transmitters zero setting done in atmosphere . Found working satisfactory.","2020-06-25T23:59:35","","Completed","2020-06-06T23:59:35","No","No","No","Internal"]
[null,null,null,11904,null,"50_15/05/2020 5:46:10 PM","2020-04-25T23:59:35","Defect,Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","2C and 4C COT dry check valve cap and handle missing ","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","Equipment Related","8.12","Medium","","","New caps received and put in place.","2021-02-23T23:59:35","DPEO200053","Completed","2021-02-02T23:59:35","No","No","No","Internal"]
[null,null,null,11905,null,"50_15/05/2020 6:29:04 PM","2020-04-25T23:59:35","Defect,Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Cargo line manifold crossover valves reported passing cargo ","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.11","Medium","","","Seat rings for all three cross-overs renewed.","2020-07-25T23:59:35","","Completed","2020-06-15T23:59:35","No","No","No","Internal"]
[null,null,null,11906,null,"50_15/05/2020 5:34:33 PM","2020-04-25T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Winches gear oil level not visible as sight glass opaque","Deck - Mooring Machinery","Mooring","Equipment Related","9.14","Medium","","","Main deck is all mooring winches gear oil checked and topped up. Gauge glasses cleaned. Glasses need renewal, no spare on board.","2020-07-25T23:59:35","","Completed","2020-07-05T23:59:35","No","No","No","Internal"]
[null,null,null,11907,null,"50_15/05/2020 5:37:23 PM","2020-04-25T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","PV breaker gauge glass spring loaded shut off valve not operational.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.28","Medium","","","Valve freed and made operational","2020-05-25T23:59:35","","Completed","2020-04-27T23:59:35","No","No","No","Internal"]
[null,null,null,11908,null,"50_15/05/2020 5:41:35 PM","2020-04-25T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Vapour manifold (P) F drain cock frozen","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.42","Medium","","","Draick cock freed","2020-07-25T23:59:35","","Completed","2020-04-26T23:59:35","No","No","No","Internal"]
[null,null,null,11909,null,"50_15/05/2020 5:52:41 PM","2020-04-25T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Fire extinguisher in Bosun store last check done in Nov 2019","LSA / FFA","Safety / LSA / FFA","Human Error","5.42","Medium","","","Extinguisher checked and inspection tag signed.","2020-04-26T23:59:35","","Completed","2020-04-26T23:59:35","No","No","No","Internal"]
[null,null,null,11910,null,"50_15/05/2020 5:55:56 PM","2020-04-25T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Spare PV valve in midship store (P) not secured","Deck - Pipe / Fittings","Safety / LSA / FFA","Behaviour Based","5.11","Low","","","To secure the PV valve on the pressure testing kit ","2020-07-25T23:59:35","","Completed","2020-04-26T23:59:35","No","No","No","Internal"]
[null,null,null,11911,null,"50_15/05/2020 6:04:12 PM","2020-04-25T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Chairs from officer's mess room being used in duty mess room ","Accommodation","General Appearance","Human Error","11.13","Low","","","Chairs to be shifted to Off mess room ","2020-07-25T23:59:35","","Completed","2020-04-28T23:59:35","No","No","No","Internal"]
[null,null,null,11912,null,"50_15/05/2020 6:13:40 PM","2020-04-25T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Anchor chain bitter end (P) hammer missing from location ","Miscellaneous","Safety / LSA / FFA","Human Error","9.22","Low","","","To put the hammer back and stencil in location - \" DO NOT REMOVE \"","2020-05-01T23:59:35","","Completed","2020-04-27T23:59:35","No","No","No","Internal"]
[null,null,null,11913,null,"50_08/05/2020 4:13:29 PM","2020-04-25T23:59:35","Defect,Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Water was found leaking from EGB into save-all tray","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","EGB isolated. Leaking HP Coil identified and leak rectified","2020-05-23T23:59:35","","Completed","2020-05-10T23:59:35","No","No","No","Internal"]
[null,null,null,11914,null,"50_08/05/2020 4:20:27 PM","2020-04-25T23:59:35","Defect,Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Fuel Oil leaking from AE#2 Fuel pump leak off line","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","All fuel pumps overhauled. no leakage observed","2020-09-23T23:59:35","","Completed","2020-05-11T23:59:35","No","No","No","Internal"]
[null,null,null,11915,null,"50_18/05/2020 3:53:21 PM","2020-04-26T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Incinerator Air damper motor found malfunctioning.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","New motor recvd at singapore. New motor fitted and incinerator operation checked. found satisfactory","2020-05-27T23:59:35","","Completed","2020-05-12T23:59:35","No","No","No","Internal"]
[null,null,null,11916,null,"50_15/05/2020 8:32:53 AM","2020-05-05T23:59:35","Observation","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","Steam leaking from 15k flange of Aux Boiler#1","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Flange bolts to be tightened","2020-05-15T23:59:35","","Completed","2020-05-06T23:59:35","No","No","No","External"]
[null,null,null,11917,null,"50_15/05/2020 6:59:10 PM","2020-05-05T23:59:35","Observation","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","Manifod drip tray drain holes were in poor condition and plugs were unable to firmly fitted. Leaking water at the time of inspection","Deck - Pipe / Fittings","MARPOL Related","Human Error","6.6","Medium","","","Drain holes, cleaned, lubricated, threads redone and fitted in place. Leak tested and found satisfactory.","2020-05-05T23:59:35","","Completed","2020-05-05T23:59:35","No","No","No","External"]
[null,null,null,12027,null,"50_31/05/2020 4:58:59 PM","2020-05-20T23:59:35","Defect","Ship Staff","Ship Staff Insp.","ME FO Booster Pump Discharge pressure guage found to be defective","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Pressure guage replaced with spare one","2020-05-27T23:59:35","","Completed","2020-05-23T23:59:35","No","No","No","Internal"]
[null,null,null,12025,null,"50_31/05/2020 4:57:09 PM","2020-05-22T23:59:35","Defect","Ship Staff","Ship Staff Insp.","ME Unit#6 Exhasut Gas Pyrometer found to be defective","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Exhasut gas pyrometers received.","2020-09-26T23:59:35","DPEO200123","Completed","2020-09-17T23:59:35","No","No","No","Internal"]
[null,null,null,12026,null,"50_31/05/2020 5:04:07 PM","2020-05-25T23:59:35","Breakdown,Defect","Ship Staff","Ship Staff Insp.","FWG High Salinity FW Recirculation solenoid valve found to be defective","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Solenoid valve  replaced with new spare one","2020-06-26T23:59:35","","Completed","2020-05-26T23:59:35","No","No","No","Internal"]
[null,null,null,13029,null,"50_12/06/2020 10:31:45 AM","2020-06-06T23:59:35","Defect,Observation","Ship Staff","Ship Staff Insp.","Coupling for Emergency hand pump operation for HH crane stbd side found corroded, wasted and holed . Same was leaking oil. ","Deck - Machinery","Cargo / Ballast Systems","Equipment Related","8.5","Very High","","","SPARES RECEIVED AND RENEWED.","2020-09-05T23:59:35","DPEO200124","Completed","2020-08-25T23:59:35","No","No","No","Internal"]
[null,null,null,13056,null,"50_30/06/2020 9:27:03 PM","2020-06-10T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","AC Compressor#1 Condenser SW inlet pressure gauge defective","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Pressure guage renewed with spare one","2020-06-11T23:59:35","","Completed","2020-06-10T23:59:35","No","No","No","Internal"]
[null,null,null,13057,null,"50_30/06/2020 9:32:01 PM","2020-06-10T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Reefer Compressor#2 belt slipping and making noise","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Belt renewed with new spare one. Motor distance adjusted.","2020-06-15T23:59:35","","Completed","2020-06-14T23:59:35","No","No","No","Internal"]
[null,null,null,13058,null,"50_30/06/2020 9:44:38 PM","2020-06-10T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Oil leaking from deck air compressor shaft lip seal","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Lip seal renewed with spare one. Compressor boxed back and put in use. No oil leak observed","2020-06-26T23:59:35","","Completed","2020-06-12T23:59:35","No","No","No","Internal"]
[null,null,null,13059,null,"50_05/07/2020 4:13:55 AM","2020-06-10T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Accomm AC Comp- Pressure switch box – cover kept opened and cover lying down\n\n","Miscellaneous","General Appearance","Equipment Related","10.32","Very High","","","switch box covers, panel covers properly fitted back","2020-06-10T23:59:35","","Completed","2020-06-10T23:59:35","No","No","No","Internal"]
[null,null,null,13060,null,"50_05/07/2020 4:16:46 AM","2020-06-10T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","#1 AC Compressor- Save all dirty with oil traces\n\n","Accommodation","General Appearance","Equipment Related","10.29","Medium","","","Save all tray cleaned and painted","2020-06-17T23:59:35","","Completed","2020-06-13T23:59:35","No","No","No","Internal"]
[null,null,null,13061,null,"50_05/07/2020 4:18:55 AM","2020-06-10T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Galley AC unit- Save all dirty – rusty with condesate water collection\n\n","Accommodation","General Appearance","Equipment Related","10.29","Medium","","","Save all tray cleaned and painted","2020-06-17T23:59:35","","Completed","2020-06-14T23:59:35","No","No","No","Internal"]
[null,null,null,13062,null,"50_05/07/2020 4:21:46 AM","2020-06-10T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","AHU room- Natural vent, Louvers frame removed and kept on the floor \n\n","Accommodation","General Appearance","Equipment Related","10.29","Medium","","","Louvre frame installed back","2020-06-10T23:59:35","","Completed","2020-06-10T23:59:35","No","No","No","Internal"]
[null,null,null,13063,null,"50_05/07/2020 4:23:37 AM","2020-06-10T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","#2 AHU\n\nTEV Inspection cover loose and in open condition – securing screws missing\n\n","Accommodation","General Appearance","Equipment Related","10.32","Very High","","","Cover put back with securing screws","2020-06-10T23:59:35","","Completed","2020-06-10T23:59:35","No","No","No","Internal"]
[null,null,null,13064,null,"50_05/07/2020 4:26:45 AM","2020-06-10T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ER Log book\n\nUMS check list complied with comments not mentioned while ER is being changed over to Unmanned\n\n","Documentation","Cert. & Docu.","Human Error","10.1","Medium","","","Comments entered in logbook","2020-06-10T23:59:35","","Completed","2020-06-10T23:59:35","No","No","No","Internal"]
[null,null,null,13065,null,"50_05/07/2020 4:32:40 AM","2020-06-10T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Water Mist System- Valve block, pump casing exterior dirty \n\n","LSA / FFA","General Appearance","Equipment Related","10.29","Medium","","","Motor, pump casing and valve block area cleaned","2020-06-17T23:59:35","","Completed","2020-06-15T23:59:35","No","No","No","Internal"]
[null,null,null,13066,null,"50_05/07/2020 5:00:49 AM","2020-06-10T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","AE 3 -LO leaks observed all over flywheel.\n\n","E/R - Aux. Engine","General Appearance","Inappropriate Procedure","10.32","Very High","","","AE No 3 : Leak rectified and area cleaned","2020-06-17T23:59:35","","Completed","2020-06-15T23:59:35","No","No","No","Internal"]
[null,null,null,13067,null,"50_05/07/2020 5:11:25 AM","2020-06-10T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Aux Boiler : Both boiler remote cables/operating lever for Gauge glass cock valves, safety valves, drain valves – at Boiler base platform (outside ECR) \n\n","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Aux Boiler : To free the seized wires, operating mechanism and ensure same can be operated remotely\n\n","2020-06-25T23:59:35","","Completed","2020-06-15T23:59:35","No","No","No","Internal"]
[null,null,null,13068,null,"50_05/07/2020 4:28:19 PM","2020-06-10T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","DO tanks- Save all/bulk head near tank drains dirty\n\n","Miscellaneous","General Appearance","Equipment Related","10.29","Medium","","","Save all tray cleaned","2020-06-10T23:59:35","","Completed","2020-06-10T23:59:35","No","No","No","Internal"]
[null,null,null,13069,null,"50_05/07/2020 4:31:04 PM","2020-06-10T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","AE#1,2- Centrufugal filter system found stopped","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","System put back in use","2020-06-10T23:59:35","","Completed","2020-06-10T23:59:35","No","No","No","Internal"]
[null,null,null,13070,null,"50_05/07/2020 4:34:30 PM","2020-06-10T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Vacuum Condensor- Save all stbd side aft area rusty/dirty \n\n","Cargo Mach.","General Appearance","Equipment Related","10.29","Medium","","","Save all tray cleaned","2020-06-16T23:59:35","","Completed","2020-06-14T23:59:35","No","No","No","Internal"]
[null,null,null,13071,null,"50_05/07/2020 4:37:59 PM","2020-06-10T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Tube light Cover- Fitting near LT cooler full of dirt/mud \n\n","Elect. Mach. & Equip.","General Appearance","Equipment Related","10.29","Medium","","","Tube light covers cleaned","2020-06-16T23:59:35","","Completed","2020-06-11T23:59:35","No","No","No","Internal"]
[null,null,null,13072,null,"50_05/07/2020 4:44:29 PM","2020-06-10T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Sea water pumps- Motors, pump exterior dirty\n\n","E/R - Pumps","General Appearance","Equipment Related","10.29","Medium","","","All motor and pump body soap washed","2020-06-25T23:59:35","","Completed","2020-06-19T23:59:35","No","No","No","Internal"]
[null,null,null,13073,null,"50_05/07/2020 4:47:35 PM","2020-06-10T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","HP circulating pump- Signs of water leakage near pump \n\n","E/R - Pumps","General Appearance","Equipment Related","10.32","Very High","","","leak rectified. save all tray cleaned","2020-07-02T23:59:35","","Completed","2020-07-15T23:59:35","No","No","No","Internal"]
[null,null,null,13074,null,"50_05/07/2020 4:53:17 PM","2020-06-10T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ME LO cooler- Area around ME LO cooler, save all dirty\n\n","E/R - Pipes/ valves & fittings","General Appearance","Equipment Related","10.29","Medium","","","Area around ME LO cooler, save all cleaned\n\n","2020-07-10T23:59:35","","Completed","2020-06-27T23:59:35","No","No","No","Internal"]
[null,null,null,13075,null,"50_07/07/2020 2:04:55 PM","2020-06-10T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Gymnasium- Mineral water bottles Stores – blocking space\n\n","Accommodation","General Appearance","Inappropriate Procedure","11.13","Low","","","Shifted to C-Deck Cable trunk","2020-06-16T23:59:35","","Completed","2020-06-11T23:59:35","No","No","No","Internal"]
[null,null,null,13076,null,"50_07/07/2020 2:21:01 PM","2020-06-10T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Fire control station\tSpare hose kept below QCV operating box/panel, blocking eacy access","LSA / FFA","Safety / LSA / FFA","Human Error","11.13","Low","","","All spare hoses shifted to safety locker.           Ensured clear/uncluttered access to panels/equipment at FC stationa always","2020-06-10T23:59:35","","Completed","2020-06-10T23:59:35","No","No","No","Internal"]
[null,null,null,13077,null,"50_07/07/2020 2:24:08 PM","2020-06-10T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Fire Man’s Suit - Noticed one suit folded and kept inside the box","LSA / FFA","Safety / LSA / FFA","Human Error","5.43","High","","","Suits hung and kept ready to ","2020-06-10T23:59:35","","Completed","2020-06-10T23:59:35","No","No","No","Internal"]
[null,null,null,13078,null,"50_05/07/2020 4:32:44 PM","2020-06-10T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Main engine Governor\n\nActuator exterior, shaft dirty\n\n","E/R - Main Engine","General Appearance","Equipment Related","10.29","Medium","","","Actuator exterior cleaned and greased","2020-06-16T23:59:35","","Completed","2020-06-13T23:59:35","No","No","No","Internal"]
[null,null,null,13079,null,"50_07/07/2020 3:33:38 PM","2020-06-10T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","China passage - Accomm block and Engine casing dirty","Accommodation","General Appearance","External Factors","11.1","High","","","oxalic acid wash carried out.","2020-06-10T23:59:35","","Completed","2020-06-19T23:59:35","No","No","No","Internal"]
[null,null,null,13080,null,"50_07/07/2020 5:03:28 PM","2020-06-10T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","EGCS  - Exhaust pipe from funnel to EGCS casing on top deck – insulation cover rusted at both ends","Miscellaneous","General Appearance","Inappropriate Procedure","10.29","Medium","","","Derusted and painted","2020-06-25T23:59:35","","Completed","2020-06-21T23:59:35","No","No","No","Internal"]
[null,null,null,13081,null,"50_07/07/2020 5:10:32 PM","2020-06-10T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ER ventilation fan casing flap - Flaps/frames look rusted ","Miscellaneous","General Appearance","External Factors","11.1","High","","","Derusted and painted","2020-08-10T23:59:35","","Completed","2020-06-20T23:59:35","No","No","No","Internal"]
[null,null,null,13082,null,"50_07/07/2020 4:21:23 PM","2020-06-10T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Aft Mooring Winches - Brake band adjusting bolts – clearances hay wire","Deck - Mooring Machinery","Mooring","Equipment Related","9.14","Medium","","","All Aft Winches adjusting bolts replaced with SS and adjusted to 3 MM clearance","2020-07-10T23:59:35","","Completed","2020-07-01T23:59:35","No","No","No","Internal"]
[null,null,null,13083,null,"50_09/07/2020 11:32:23 AM","2020-06-10T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","EGCS/ Scrubber house - All areas/frames, platform dirty – no indication of any one had taken house keeping since last few months!!","Miscellaneous","General Appearance","Human Error","10.29","Medium","","","All areas have been sweeped and mopped. Regular rounds being taken to maintain cleanliness.","2020-07-02T23:59:35","","Completed","2020-06-16T23:59:35","No","No","No","Internal"]
[null,null,null,13084,null,"50_05/07/2020 4:56:40 PM","2020-06-10T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ME Full intermediate shaft rusty ","E/R - Main Engine","General Appearance","Equipment Related","10.29","Medium","","","Shaft cleaned and greased","2020-07-10T23:59:35","","Completed","2020-06-29T23:59:35","No","No","No","Internal"]
[null,null,null,13085,null,"50_09/07/2020 11:48:34 AM","2020-06-10T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Accommodation Gangway - Port side Gangway oil filter, auto drain both rusted and wasted","Deck - Machinery","General Appearance","External Factors","5.47","Medium","","","Renewed Complete Filter Assembly","2020-06-25T23:59:35","","Completed","2020-06-29T23:59:35","No","No","No","Internal"]
[null,null,null,13086,null,"50_09/07/2020 3:10:56 PM","2020-06-10T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Fwd Hyd system tank - Air filter unit fully rusted ","Deck - Mooring Machinery","General Appearance","External Factors","11.4","Very High","","","Air filter unit taken out, maintenance carried out and painted","2020-07-02T23:59:35","","Completed","2020-07-01T23:59:35","No","No","No","Internal"]
[null,null,null,17517,null,"50_15/01/2021 11:48:35 PM","2020-06-10T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Lying haphazard, piston rings not oiled and kept.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Completed","2020-06-24T23:59:35","","Completed","2020-06-16T23:59:35","No","No","No","Internal"]
[null,null,null,17518,null,"50_16/01/2021 12:30:23 AM","2020-06-10T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Centrifugal filter not installed.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Installed","2020-06-24T23:59:35","","Completed","2020-06-21T23:59:35","No","No","No","Internal"]
[null,null,null,17519,null,"50_16/01/2021 12:35:30 AM","2020-06-10T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Jacket water cooler- aft of ME on cylinder head platform. The unit looks very dirty - water leaking marks from top to second platform and salt deposits. looks like no one is bothered to even have a look.","E/R - Main Engine","Eng. / Strg. Comp.","Behaviour Based","10.32","Very High","","","Leaks rectified","2020-06-24T23:59:35","","Completed","2020-06-23T23:59:35","No","No","No","Internal"]
[null,null,null,17520,null,"50_16/01/2021 12:38:25 AM","2020-06-10T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Cross head LO pump- No.1 pump show signs of LO leaks from seals.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Checked and leak rectified.","2020-08-10T23:59:35","","Completed","2020-07-15T23:59:35","No","No","No","Internal"]
[null,null,null,17521,null,"50_16/01/2021 12:42:23 AM","2020-06-10T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Entablature exterior dirty with oil streaks all over.","E/R - Main Engine","Eng. / Strg. Comp.","Behaviour Based","10.29","Medium","","","Entablature cleaned.","2020-06-17T23:59:35","","Completed","2020-06-15T23:59:35","No","No","No","Internal"]
[null,null,null,17522,null,"50_16/01/2021 12:46:15 AM","2020-06-10T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Scrubber SW pump- area of SW pump- tank top, pipelines, gratings, bulkhead- Dirty","E/R - Pumps","Eng. / Strg. Comp.","Behaviour Based","10.29","Medium","","","Area and pipelines soap washed.","2020-07-10T23:59:35","","Completed","2020-07-10T23:59:35","No","No","No","Internal"]
[null,null,null,17523,null,"50_16/01/2021 12:52:49 AM","2020-06-10T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Incolube unit- Noticed in alarm condition- any trouble?","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Shore technician help received. Fault rectified","2020-06-10T23:59:35","","Completed","2020-06-12T23:59:35","No","No","No","Internal"]
[null,null,null,17524,null,"50_16/01/2021 12:56:16 AM","2020-06-10T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","AE #3-  Fuel nozzles supposed to replace at 4000 hrs","E/R - Aux. Engine","Eng. / Strg. Comp.","Behaviour Based","10.12","Very High","","","Sufficiend spares onboard","2020-06-24T23:59:35","","Completed","2020-06-13T23:59:35","No","No","No","Internal"]
[null,null,null,17525,null,"50_16/01/2021 1:00:30 AM","2020-06-10T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","AE 1 & 2- Centrifugal filters- Oilmax","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","System put in use","2020-06-10T23:59:35","","Completed","2020-06-10T23:59:35","No","No","No","Internal"]
[null,null,null,17526,null,"50_16/01/2021 1:05:06 AM","2020-06-10T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Officers Smoke room- Music system lying loose- not lashed, wires lying haphazard not clubed and routed properly.","Accommodation","General Appearance","Behaviour Based","11.13","Low","","","Music system secured. Cleaned and squared up. Continuous maintenance of cleanliness carried out.","2020-06-17T23:59:35","","Completed","2020-06-11T23:59:35","No","No","No","Internal"]
[null,null,null,17527,null,"50_16/01/2021 1:08:21 AM","2020-06-10T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Reported #1 COT goes offline- once a while.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.8","Medium","","","Error rectified.","2020-06-17T23:59:35","","Completed","2020-09-11T23:59:35","No","No","No","Internal"]
[null,null,null,17528,null,"50_16/01/2021 1:12:54 AM","2020-06-10T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Laundry room- Observed very hot- on checking noticed drying room thermostat kept at 70 Deg C ! !","Accommodation","Crew Management","Behaviour Based","11.13","Low","","","Temperature setting reduced to 35 Deg C","2020-06-10T23:59:35","","Completed","2020-06-10T23:59:35","No","No","No","Internal"]
[null,null,null,17529,null,"50_16/01/2021 1:15:35 AM","2020-06-10T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Foam room- found one light fused.","Elect. Mach. & Equip.","Safety / LSA / FFA","Behaviour Based","11.6","Medium","","","Renewed","2020-06-10T23:59:35","","Completed","2020-06-10T23:59:35","No","No","No","Internal"]
[null,null,null,17530,null,"50_16/01/2021 1:20:09 AM","2020-06-10T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","WO Tank vent on deck- Dirty cloth tied around the vent to prevent steam/oily vapours- this will require any their part comment.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Behaviour Based","11.4","Very High","","","Cloth removed and cleaned regularly.","2020-06-17T23:59:35","","Completed","2020-06-13T23:59:35","No","No","No","Internal"]
[null,null,null,17531,null,"50_16/01/2021 1:26:28 AM","2020-06-10T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Elevator- floor mat/ Linoleum very dirty.","Accommodation","General Appearance","Behaviour Based","11.13","Low","","","Renewed","2020-07-10T23:59:35","","Completed","2020-06-17T23:59:35","No","No","No","Internal"]
[null,null,null,17532,null,"50_16/01/2021 1:23:02 AM","2020-06-10T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","T/C Suction filter casing- Rusty and dirty.","E/R - Main Engine","Eng. / Strg. Comp.","Behaviour Based","11.3","Medium","","","Completed","2020-07-10T23:59:35","","Completed","2020-06-30T23:59:35","No","No","No","Internal"]
[null,null,null,13030,null,"50_30/06/2020 9:36:44 PM","2020-06-10T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Workshop grinding machine imbalanced. ","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","New bearings received. Grinding m/c overhauled,bearings renewed.","2020-07-10T23:59:35","","Completed","2020-08-29T23:59:35","No","No","No","Internal"]
[null,null,null,13031,null,"50_30/06/2020 9:47:38 PM","2020-06-10T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ME Intermediate shaft rusty","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Shaft cleaned/derusted,then light coated with grease.","2020-07-10T23:59:35","","Completed","2020-07-09T23:59:35","No","No","No","Internal"]
[null,null,null,13032,null,"50_30/06/2020 9:51:10 PM","2020-06-10T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Engine room tank top found dirty","Miscellaneous","General Appearance","Equipment Related","10.29","Medium","","","E/R tank top area to be cleaned and painted.","2020-07-10T23:59:35","","Completed","2020-07-17T23:59:35","No","No","No","Internal"]
[null,null,null,13033,null,"50_05/07/2020 4:30:12 AM","2020-06-10T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ME Spare fuel valves- To overhaul,pressure test and keep ready to use.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.12","Very High","","","ME Spare fuel valves overhauling is in progress. total 15 nos of valves.","2020-09-10T23:59:35","","Completed","2020-11-01T23:59:35","No","No","No","Internal"]
[null,null,null,13034,null,"50_05/07/2020 4:44:55 AM","2020-06-10T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","EGCS sea water chest suction valve remote operating unit, no dates of last tried out .\n\n","Miscellaneous","Cert. & Docu.","Human Error","10.12","Very High","","","EGCS sea water chest suction valve remote operating unit-JOB INCLUDED IN PMS,tred out on 17-July-2020.\n\n\n\n","2020-06-10T23:59:35","","Completed","2020-07-12T23:59:35","No","No","No","Internal"]
[null,null,null,13035,null,"50_05/07/2020 5:05:13 AM","2020-06-10T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","AE #3 : Crank case looks getting pressurized – Sump dip stick missing and kept opened\n\n","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Modified c/case vent line fabricated and fitted.Now,c/case not pressurised.","2020-07-10T23:59:35","","Completed","2020-07-10T23:59:35","No","No","No","Internal"]
[null,null,null,13036,null,"50_05/07/2020 4:58:42 PM","2020-06-10T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Bilge/Tank top found in dirty condition","Miscellaneous","General Appearance","Equipment Related","10.29","Medium","","","tank top cleaned by soap water.","2020-07-10T23:59:35","","Completed","2020-07-02T23:59:35","No","No","No","Internal"]
[null,null,null,13037,null,"50_05/07/2020 5:01:15 PM","2020-06-10T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","AE #1- overhaul/ decarb due.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.12","Very High","","","A/E#1 DECARB STARTED,JOB IS IN PROGRESS.","2020-10-10T23:59:35","","Completed","2020-11-15T23:59:35","No","No","No","Internal"]
[null,null,null,13039,null,"50_07/07/2020 3:36:37 PM","2020-06-10T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Common deck Store\tWater tight doors, not closing properly","Accommodation","Structural Condn. / WT integrity ","External Factors","11.3","Medium","","","Repaired and proper tightening ensured. Chalk test carried out and found satisfactory. All other WT doors checked and chalk tested.","2020-06-17T23:59:35","","Completed","2020-07-09T23:59:35","No","No","No","Internal"]
[null,null,null,13040,null,"50_07/07/2020 4:14:04 PM","2020-06-10T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Natural vents – covers of various spce at Various stages of corrossion","Accommodation","General Appearance","External Factors","11.3","Medium","","","Spot Derusted and Painted","2020-08-10T23:59:35","","Completed","2020-08-21T23:59:35","No","No","No","Internal"]
[null,null,null,13041,null,"50_07/07/2020 4:16:40 PM","2020-06-10T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Tube light fittings\tFittings on Accommodation front – facing main deck and on other acoomm decks the fitting angle farmes are rusted/corroded","Accommodation","General Appearance","External Factors","11.16","Low","","","Derusted and painted with 2 coats of primer and finish coat","2020-07-10T23:59:35","","Completed","2020-07-09T23:59:35","No","No","No","Internal"]
[null,null,null,13043,null,"50_07/07/2020 4:18:28 PM","2020-06-10T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Pump room blowers\tBlower Stay pipes/flange ends rusty ","Deck - Pipe / Fittings","General Appearance","External Factors","11.14","Medium","","","Thoroughly derusted and painted with 2 coats of primer and finish coat","2020-07-10T23:59:35","","Completed","2020-07-08T23:59:35","No","No","No","Internal"]
[null,null,null,13044,null,"50_07/07/2020 5:13:06 PM","2020-06-10T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Funnel casing - Dirty/rust weepings","Miscellaneous","General Appearance","External Factors","11.1","High","","","Oxalic acid wash followed by high pressure FW wash carried out","2020-08-10T23:59:35","","Completed","2020-07-09T23:59:35","No","No","No","Internal"]
[null,null,null,13045,null,"50_09/07/2020 11:38:23 AM","2020-06-10T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Main deck\tPipe U bolts - Few bolts found rusted ","Deck - Pipe / Fittings","General Appearance","External Factors","11.5","Medium","","","Derusting and painting in progress. New observation raised.","2021-05-26T23:59:35","","Completed","2021-04-26T23:59:35","No","No","No","Internal"]
[null,null,null,13046,null,"50_09/07/2020 11:41:22 AM","2020-06-10T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Aft Stern Light - Frame rusted, base corroded","Deck - Pipe / Fittings","General Appearance","External Factors","4.8","Medium","","","Frame derusted and painted.","2020-07-10T23:59:35","","Completed","2020-08-29T23:59:35","No","No","No","Internal"]
[null,null,null,13047,null,"50_09/07/2020 11:43:51 AM","2020-06-10T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Hydraulic remote control valve boxes on deck - Box lips rusted and getting wasted","Deck - Pipe / Fittings","General Appearance","External Factors","11.3","Medium","","","Rusted boxes Derusted and painted. Wasted Sections renewed.","2020-08-10T23:59:35","","Completed","2020-08-14T23:59:35","No","No","No","Internal"]
[null,null,null,13048,null,"50_09/07/2020 11:51:02 AM","2020-06-10T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","PV valves - Few PV valves reported leaking","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.19","High","","","Temporary repair carried out and leaks arrested. Require shore servicing for permanent solution","2020-09-10T23:59:35","","Completed","2020-10-07T23:59:35","No","No","No","Internal"]
[null,null,null,13049,null,"50_09/07/2020 3:03:30 PM","2020-06-10T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Wind Sock - Frame/pipe rusted","Deck - Pipe / Fittings","General Appearance","External Factors","11.4","Very High","","","Derusted and painted with 2 coats of primer and full finish coat","2020-07-10T23:59:35","","Completed","2020-07-08T23:59:35","No","No","No","Internal"]
[null,null,null,13050,null,"50_09/07/2020 3:00:50 PM","2020-06-10T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Deck outfittings - At various stages of corrosion ","Deck - Pipe / Fittings","General Appearance","External Factors","11.5","Medium","","","Maintenance in progress. Fresh observation raised.","2021-05-26T23:59:35","","Completed","2021-04-26T23:59:35","No","No","No","Internal"]
[null,null,null,13051,null,"50_09/07/2020 3:08:20 PM","2020-06-10T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Fwd Hydraulic system tank - Top area rusted","Deck - Mooring Machinery","General Appearance","External Factors","11.3","Medium","","","Derusted and full coat painted","2020-07-10T23:59:35","","Completed","2020-07-05T23:59:35","No","No","No","Internal"]
[null,null,null,13052,null,"50_09/07/2020 11:36:22 AM","2020-06-10T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Main Deck - Cable tray running parallel to cargo pipes at various stges of corossion","Deck - Pipe / Fittings","General Appearance","External Factors","11.5","Medium","","","Maintenance in progress. Fresh observation raised.","2021-04-25T23:59:35","","Completed","2021-04-26T23:59:35","No","No","No","Internal"]
[null,null,null,13054,null,"50_30/06/2020 9:20:05 PM","2020-06-10T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Condenser Cooling SW inlet Pressure gauge defective","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Pressure guage renewed with new spare one","2020-06-11T23:59:35","","Completed","2020-06-10T23:59:35","No","No","No","Internal"]
[null,null,null,13055,null,"50_30/06/2020 9:24:25 PM","2020-06-10T23:59:35","Breakdown","Owner / Marine / Tech. Suptd.","Suptd. Insp.","AC Compressor#1 Coupling found broken and compressor could not be used","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","New Coupling received and installed on new AC Compressor. Compressor tried out and put in use","2020-06-26T23:59:35","","Completed","2020-06-20T23:59:35","No","No","No","Internal"]
[null,null,null,13087,null,"50_18/06/2020 9:31:01 AM","2020-06-13T23:59:35","Defect,Observation","Ship Staff","Ship Staff Insp.","Loadicator not going online . Showing error online file expired, not coonected ","Miscellaneous","Cargo / Ballast Systems","Equipment Related","8.8","Medium","","","Rosemount system was restarted 2 times and Loadicator was restarted 2 times . Now the Loadicator is going online except 1P cot ","2020-08-12T23:59:35","","Completed","2020-06-14T23:59:35","No","No","No","Internal"]
[null,null,null,13053,null,"50_23/06/2020 6:25:53 PM","2020-06-18T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Ship Staff Insp.","CCTV cameras not installed in following location :                 1)      2 nos in Bridge (Facing BCC and Radio/Chart tables).\n\n2)      1 no in Cargo control room facing Cargo Console.\n\n3)      2 nos. in ECR (Facing switch board and ECR Console. \n\n4)      1 no. mid section of bridge facing deck area to cover entire deck (if camera is not fitted on bridge wings).\n\n5)      1 no inside scrubber housing (if vessel fitted with scrubber)\n\n","Miscellaneous","ISPS Related","Equipment Related","7.12","High","","","CCTV cameras Installed in designated locations and Commissioned.","2020-09-25T23:59:35","","Completed","2020-09-25T23:59:35","No","No","No","Internal"]
[null,null,null,13398,null,"50_31/07/2020 4:30:05 PM","2020-07-12T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","At STBD manifold, some bolts were found short.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Industry Issue","8.3","Very High","","","Short Bolts replaced with Longer Bolts","2020-08-15T23:59:35","","Completed","2020-07-15T23:59:35","No","No","No","Internal"]
[null,null,null,13399,null,"50_25/07/2020 4:14:22 PM","2020-07-14T23:59:35","Observation","Owner / Marine / Tech. Suptd.","ISM Audit","Numerous used parts from dry dock to be off landed","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Used parts and scrap metal landed at Yiu Lian drydock.","2021-03-05T23:59:35","","Completed","2021-02-24T23:59:35","No","No","No","Internal"]
[null,null,null,13400,null,"50_25/07/2020 4:16:29 PM","2020-07-14T23:59:35","Observation","Owner / Marine / Tech. Suptd.","ISM Audit","At STBD manifold, some bolts were found short. Same to be renewed at the earliest","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.3","Very High","","","Short bolts replaced with longer bolts","2020-11-26T23:59:35","","Completed","2020-07-15T23:59:35","No","No","No","Internal"]
[null,null,null,13401,null,"50_25/07/2020 4:18:01 PM","2020-07-14T23:59:35","Observation","Owner / Marine / Tech. Suptd.","ISM Audit","Numerous leak stains found on Main Engine entablature","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Fuel oil leakage from no.2 unit rectified. complete entablature thoroughly cleaned. areas to be painted at the next convenient opportunity.","2020-09-26T23:59:35","","Completed","2020-08-31T23:59:35","No","No","No","Internal"]
[null,null,null,13402,null,"50_25/07/2020 4:21:07 PM","2020-07-14T23:59:35","Defect,Observation","Owner / Marine / Tech. Suptd.","ISM Audit","#2 Main feed Water Pump discharge pressure gauge found defective","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","discharge pressure guage replaced by new spare.","2020-07-27T23:59:35","","Completed","2020-07-17T23:59:35","No","No","No","Internal"]
[null,null,null,13403,null,"50_25/07/2020 4:33:43 PM","2020-07-14T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Reefer compresoor - Icing observed in suction line","Accommodation","Eng. / Strg. Comp.","Equipment Related","5.29","High","","","Filter/drier renewed. Meat room,fish room line filter cleaned. solenoid valve cleaned.","2020-07-24T23:59:35","","Completed","2020-07-18T23:59:35","No","No","No","Internal"]
[null,null,null,13404,null,"50_25/07/2020 4:36:42 PM","2020-07-14T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","#2 AC Compressor - Newly supplied Compressor, reported oil seal leaks","Accommodation","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Mechanical seal flange opened-up,area cleaned thoroughly and fitted back.At present,Negligible leakage only, acceptable.","2020-07-21T23:59:35","","Completed","2020-07-20T23:59:35","No","No","No","Internal"]
[null,null,null,13405,null,"50_25/07/2020 4:38:40 PM","2020-07-14T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","EGG- Exhaust gas leakage from EGB foundation.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Leakage identified and repaired. ","2020-09-14T23:59:35","","Completed","2020-08-09T23:59:35","Yes","No","No","Internal"]
[null,null,null,13406,null,"50_25/07/2020 4:40:01 PM","2020-07-14T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","EGB Soot blowers - To clean and maintain tidy. Soot blower Motor exterior dirty","E/R - Boiler","General Appearance","Equipment Related","10.29","Medium","","","Soot blowers and surrounding area cleaned.","2020-07-21T23:59:35","","Completed","2020-07-17T23:59:35","No","No","No","Internal"]
[null,null,null,13407,null,"50_25/07/2020 4:29:16 PM","2020-07-14T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","LSMGO bunker line valve not gear operated","Deck - Pipe / Fittings","MARPOL Related","Equipment Related","6.7","High","","","new gear operated valves received. Butterfly valves replaced by new gear operated valves.","2020-07-30T23:59:35","","Completed","2020-07-23T23:59:35","No","No","No","Internal"]
[null,null,null,13408,null,"50_25/07/2020 4:35:13 PM","2020-07-14T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","#1 AC Compressor - SW line press gauge fitted lose","Accommodation","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","New spare pr. gauge with correct size rim, fitted in place and secured.","2020-07-24T23:59:35","","Completed","2020-07-23T23:59:35","No","No","No","Internal"]
[null,null,null,13409,null,"50_25/07/2020 4:42:43 PM","2020-07-14T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ME exh damper - To rectify the leaks – else service/control air compressor shall be loaded for long. ","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Damper control air line leakage rectified.","2020-07-21T23:59:35","","Completed","2020-08-02T23:59:35","No","No","No","Internal"]
[null,null,null,13410,null,"50_25/07/2020 4:44:04 PM","2020-07-14T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","EGB- To clean and paint - Save alls, adjacent bulkheads, laggings, pipe lines dirty","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Savealls, adjacent bulkheads, laggings and pipelines cleaned thoroughly, then painted.","2020-08-14T23:59:35","","Completed","2020-08-01T23:59:35","No","No","No","Internal"]
[null,null,null,13411,null,"50_25/07/2020 4:45:18 PM","2020-07-14T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","AE #3 - To check for leak sources and rectify ","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","A/E#3 SOLEOID VALVE OVERHAULED,O-RINGS RENEWED. LEAKAGE ARRESTED.","2020-08-14T23:59:35","","Completed","2020-08-03T23:59:35","No","No","No","Internal"]
[null,null,null,13412,null,"50_25/07/2020 4:46:50 PM","2020-07-14T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Steam line - To open and check the safety valve at next opportunity. 6 Kg service line relief valve leaking","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Safety valve overhauled, pressure tested and put back. leakage stopped.","2020-08-28T23:59:35","","Completed","2020-08-18T23:59:35","No","No","No","Internal"]
[null,null,null,13413,null,"50_25/07/2020 4:48:37 PM","2020-07-14T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Aft Hydraulic system - Containers kept to hold the leaks, flange to be opened, check and if required to cut and replace section of pipe with new flanges. LO cooler SW pipe flanges leaking.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Both s.w.inlet & outlet pipes for cooler found leaking, same removed,weld repaired and put back.","2020-08-09T23:59:35","","Completed","2020-08-12T23:59:35","No","No","No","Internal"]
[null,null,null,13414,null,"50_25/07/2020 4:41:10 PM","2020-07-14T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","AE #3 To check and rectify - Exhaust gas leaks suspected in the uptakes above EGB platform","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Job created in Refman for d/dock repair.Exhaust gas leakage from A/E#3 uptake-from 2nd dk top,IG platform.staging required for 2nd dk.","2020-07-21T23:59:35","","Completed","2020-07-27T23:59:35","Yes","No","No","Internal"]
[null,null,null,13415,null,"50_25/07/2020 4:50:05 PM","2020-07-14T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Steering room - Same to be installed, flange bolts tightness to be checked, to avoid pipe damages. Pipes on the ceiling, which were opened at DD for EGCS installation – hyd lines, fire line – most of the clamps are not fitted back, vibrations reported","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Hyd.line supports/clamps tightened.","2020-07-28T23:59:35","","Completed","2020-07-22T23:59:35","No","No","No","Internal"]
[null,null,null,13416,null,"50_25/07/2020 4:51:28 PM","2020-07-14T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Incinerator- DO service tank, Quick closing valve leaking","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Diesel oil leakage rectified.","2020-07-28T23:59:35","","Completed","2020-07-22T23:59:35","No","No","No","Internal"]
[null,null,null,13417,null,"50_25/07/2020 4:56:44 PM","2020-07-14T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Atmos condensor- Sea water leaks from flanges observed","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Atmos.condenser sea water leakage rectified.","2020-07-21T23:59:35","","Completed","2020-08-19T23:59:35","No","No","No","Internal"]
[null,null,null,13418,null,"50_25/07/2020 4:58:06 PM","2020-07-14T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","AE #1- ESM has one alarm lit ","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","In consultation with Technician&Tech.suptd, ESM module renewed. secondary power from Bridge battery charge/discharge panel was off,same put-on. alarm disappeared.","2020-07-15T23:59:35","","Completed","2020-08-03T23:59:35","No","No","No","Internal"]
[null,null,null,13419,null,"50_25/07/2020 4:59:30 PM","2020-07-14T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Main Engine - Old plugged cylinder lubrication holes in the liner has water leakages from few units ","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Water leakage from old plugged cyl.quills rectified.","2020-09-09T23:59:35","","Completed","2020-08-02T23:59:35","No","No","No","Internal"]
[null,null,null,13420,null,"50_25/07/2020 5:02:26 PM","2020-07-14T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Fwd LT cooler Sea water inlet valve leaks fom flange observed","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Fwd L.T.Cooler sea water leakage from flange rectified.","2020-08-14T23:59:35","","Completed","2020-08-19T23:59:35","No","No","No","Internal"]
[null,null,null,13421,null,"50_25/07/2020 5:05:39 PM","2020-07-14T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ME Aft Air cooler - Water washing line, valve leaking","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Leaking valve replaced by spare.","2020-07-29T23:59:35","","Completed","2020-08-02T23:59:35","No","No","No","Internal"]
[null,null,null,13422,null,"50_25/07/2020 4:54:02 PM","2020-07-14T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","EGCS- No spare for air seal motor","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.12","Very High","",""," RO raised for new spare motor.","2020-07-21T23:59:35","","Completed","2020-07-18T23:59:35","No","No","No","Internal"]
[null,null,null,13423,null,"50_25/07/2020 5:12:15 PM","2020-07-14T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Spares Invetory updates- Pending for physical checks and update in PAL","Miscellaneous","Cert. & Docu.","Behaviour Based","10.12","Very High","","","Physically checked and updated in PAL PMS.\n\n\n\n\n\n\n\n","2020-08-14T23:59:35","","Completed","2020-08-19T23:59:35","No","No","No","Internal"]
[null,null,null,13424,null,"50_25/07/2020 5:14:31 PM","2020-07-14T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","LED lights upgrade in ER - Still few pending","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","All tube lights replaced by LED lights. New RO raised for lights and fittings.","2020-08-14T23:59:35","","Completed","2020-08-10T23:59:35","No","No","No","Internal"]
[null,null,null,13425,null,"50_29/07/2020 4:07:46 PM","2020-07-14T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Galley - Dish washer not in use","Accommodation","MLC Related","Equipment Related","11.16","Low","","","Drain line has been cleared and water supply confirmed.Put in-use.","2020-08-14T23:59:35","","Completed","2020-08-29T23:59:35","No","No","No","Internal"]
[null,null,null,13426,null,"50_25/07/2020 4:55:33 PM","2020-07-14T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Work shop - Welding curtains observed, were of non approved type","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","5.25","Medium","","","New welding curtains received from Unitor installed. RO raised for 4 more pcs.","2020-07-21T23:59:35","","Completed","2020-08-21T23:59:35","No","No","No","Internal"]
[null,null,null,13427,null,"50_25/07/2020 5:09:47 PM","2020-07-14T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","EGCS - Engine load is showing differently on ME remote gauge in ECR and on EGCS panel – 10% more – hence GECS operates on higher load","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","M/E Load transmitter for EGCS has been identified in ECR panel and potentiometer adjusted,so that mainengine stop condition, load shows zero at EGCS.","2020-07-21T23:59:35","","Completed","2020-09-07T23:59:35","No","No","No","Internal"]
[null,null,null,13428,null,"50_25/07/2020 4:10:51 PM","2020-07-14T23:59:35","Observation","Owner / Marine / Tech. Suptd.","ISM Audit","Leak noted at FO Booster Pump pressure switch","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Leak rectified at ME FO Booster pump pressure switch","2020-07-27T23:59:35","","Completed","2020-07-16T23:59:35","No","No","No","Internal"]
[null,null,null,13429,null,"50_25/07/2020 4:25:35 PM","2020-07-14T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","E/R Sky light door was kept opened during cargo discharge ops","Miscellaneous","Eng. / Strg. Comp.","Behaviour Based","5.1","Very High","","","sky light door shut immediately","2020-07-14T23:59:35","","Completed","2020-07-14T23:59:35","No","No","No","Internal"]
[null,null,null,13430,null,"50_29/07/2020 4:10:54 PM","2020-07-14T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","SIP natural vents - All natural vents marked as ‘SIP’ were observed in open condition – during cargo disch ops","Accommodation","Safety / LSA / FFA","Human Error","5.1","Very High","","","All SIPs were checked and open ones were shut immediately. Crew briefed regarding same and a practice of checking of the SIPs prior arrival port was put in place","2020-07-14T23:59:35","","Completed","2020-07-14T23:59:35","No","No","No","Internal"]
[null,null,null,13431,null,"50_29/07/2020 4:14:29 PM","2020-07-14T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","COP  - COP #3 leaking from top seal","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.44","High","","","Top seal was slackened and cleaned. Found not leaking. The leak was form the Cooling line connection which was slack due to vibration. Same tightened and clean-up carried out.","2020-07-21T23:59:35","","Completed","2020-07-17T23:59:35","No","No","No","Internal"]
[null,null,null,13432,null,"50_29/07/2020 4:17:53 PM","2020-07-14T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","House keeping - House keeping in public places – Smoke rooms, dining spaces, change rooms, Laundry has scope for improvements","Accommodation","MLC Related","Behaviour Based","11.13","Low","","","All Public places cleaned, squared-up and orderly arranged.All dustbins emptied on regular basis. Continuous maintenance of cleanliness in progress.","2020-07-29T23:59:35","","Completed","2020-07-21T23:59:35","No","No","No","Internal"]
[null,null,null,13433,null,"50_25/07/2020 4:31:46 PM","2020-07-14T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","COP #3 leaking from top seal","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.44","High","","","top seal flange removed and sea inspected and cleaned. Leak was from cooling line pipe connection. Pipe connection tightened properly","2020-07-21T23:59:35","","Completed","2020-07-17T23:59:35","No","No","No","Internal"]
[null,null,null,13042,null,"50_12/06/2020 12:33:20 PM","2020-07-14T23:59:35","Breakdown,Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","SAAB tank radar system - 5P and 3P reported error in sounding level","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.8","Medium","","","Troubleshooting carried out and fault rectified by ETO.","2020-07-21T23:59:35","","Completed","2020-07-18T23:59:35","No","No","No","Internal"]
[null,null,null,13856,null,"50_17/08/2020 3:20:17 PM","2020-08-12T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Personnel Transfer Basket - During 3M inspection, it was observed that one of the strands have broken off from a splice at the bottom frame. Other splices checked and found to be brittle and easily breakable.","Miscellaneous","Safety / LSA / FFA","Equipment Related","5.47","Medium","","","New PTB received while passing Singapore. Old PTB replaced by new one. ","2020-09-25T23:59:35","","Completed","2020-08-20T23:59:35","No","No","No","Internal"]
[null,null,null,13857,null,"50_17/08/2020 3:13:53 PM","2020-08-12T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Lifeboat - Brake release handle eyes for securing remote launching wire shieves found wasted.","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.28","Very High","","","The brake handles were removed and taken to E/rm workshop. The wasted eyes were cropped and new eyes fabricated and fitted. The handles were brought back and fitted in place.","2020-08-17T23:59:35","","Completed","2020-08-13T23:59:35","No","No","No","Internal"]
[null,null,null,20789,null,"50_03/09/2021 12:56:45 PM","2020-08-19T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Sound powered telephone from Emergency manouvering flat is not working","Miscellaneous","Communication","Equipment Related","10.39","High","","","Found the dynamometer faulty same interchanged from CE Cabin.","2021-11-20T23:59:35","DPEO 210181","Completed","2021-08-29T23:59:35","No","No","No","Internal"]
[null,null,null,16463,null,"50_04/01/2021 11:25:22","2020-08-31T23:59:35","Observation","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","The properly completed MSMP Register was not shown during the\n\ninspection. The MSMP Register was provided with part C only. As per MEG 4 item 1.9.2.7\n\nMSMPR would have a representative table for each MSMP part not only part C.","Documentation","Cert. & Docu.","Inappropriate Procedure","9.2","Very High","","","Ships specific MSMP is in line with MEG-4 requirements. It is to be noted that\n\nthe information for each parts have been elaborated chapter wise which has not been\n\ntabulated again in the part G except Part C. For guidance, item no. 1.9.2.7- Part G- Mooring\n\nsystem Management plan register due to the nature of brief explanation of each part right\n\nfrom part A to Part G in accordance to the MEG-4 guidelines, all Parts( Part A to G) are\n\nexplained with in the each part section.","2020-09-14T23:59:35","","Completed","2020-09-07T23:59:35","No","No","No","External"]
[null,null,null,16464,null,"50_04/01/2021 11:14:16","2020-08-31T23:59:35","Observation","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","The GPS sensor No 1 showed transverse deviation of the vessel position (approx. half of the vessel breadth) on the port side ECDIS. After changing of the position sensor to GPS No2 the vessel position was aligned with the actual vessel position along a jetty. The sensor position for GPS No1 showed red indication for one of several items applicable to GPS sensor position in the ECDIS menu. ","Navigation - ECDIS","Navigation","Equipment Related","4.17","Very High","","","Corrective Action & Preventive Action: The position sensor of the ECDIS was immediately\n\nchanged to DGPS-2 during the course of inspection and it was observed that the DGPS position on ECDIS was aligned with actual position of the vessel with respect to jetty as witnessed by the inspector. DGPS 1 was restarted and its position was found matching with GPS2 and noted to be accurate. Subsequently there was no alarm indication on ECDIS anymore.","2020-09-07T23:59:35","","Completed","2020-08-31T23:59:35","No","No","No","External"]
[null,null,null,16465,null,"50_04/01/2021 11:28:28","2020-08-31T23:59:35","Observation","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","The bunkering checklist used for bunkering of low sulphur marine gas\n\noil dated 15 June 2020 was not provided with measurements of benzene content. Not\n\napplicable statement was written on the check list. The bunkering checklist had tables for\n\nbenzene checking.","Documentation","Cert. & Docu.","Knowledge Based","10.8","Medium","","","Root Cause: Benzene content in LSMGO tanks were checked during bunkering operation and noted to be zero. However inadvertently the officer in charge has recorded the benzene content figure as N/A in the checklist instead of Zero (0).\n\nCorrective Action and Preventive Action: The said checklist has been corrected with actual\n\nfigure zero (0). Importance of correct entries in checklists and proper recordkeeping have been\n\nhighlighted and discussed by safety officer with all onboard to their understanding.\n\nCrew were reiterated in correct filling of checklists. We wish to confirm that record keeping and checklist filling will be executed properly with due diligence. Superintendents will monitor\n\nvessel’s compliance during their shipboard visits.","2020-10-31T23:59:35","","Completed","2020-09-13T23:59:35","No","No","No","External"]
[null,null,null,14215,null,"50_29/09/2020 3:48:26 PM","2020-09-05T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Manifold - No 4 Manifold valve Portside observed leaking during discharge operation","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.11","Medium","","","Damaged seat ring of the valve renewed.","2020-10-05T23:59:35","","Completed","2020-10-02T23:59:35","No","No","No","Internal"]
[null,null,null,17533,null,"50_18/01/2021 12:05:44","2020-09-15T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Mooring Audit","Mooring: Grease of cleat rollers on forecastle deck was dried up and rollers were frozen.","Deck - Mooring Machinery","Mooring","Inappropriate Procedure,Knowledge Based","9.18","Low","","","All cleat rollers and mooring equipment  thoroughly greased and checked for free operation.","2020-12-14T23:59:35","","Completed","2020-09-19T23:59:35","No","No","No","Internal"]
[null,null,null,17538,null,"50_18/01/2021 12:14:20","2020-09-15T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Nav Audit / Verification","NAV: Emergency light provided for GMDSS panel was not operational at the time of inspection.","Navigation - GMDSS & Communication","Navigation","Equipment Related,Human Error","4.21","High","","","Wiring of the emergency light was checked and found disconnected from power source. Same was connected immediately and light made operational.","2020-11-14T23:59:35","","Completed","2020-09-19T23:59:35","No","No","No","Internal"]
[null,null,null,14211,null,"50_05/10/2020 5:49:52 PM","2020-09-15T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Mooring winch -Mooring winch #2 hydraulic oil leakage from inlet line flange ","Deck - Mooring Machinery","Mooring","Equipment Related","11.4","Very High","","","Leakage rectified by replacing O-ring.","2020-09-30T23:59:35","","Completed","2020-10-28T23:59:35","No","No","No","Internal"]
[null,null,null,14212,null,"50_05/10/2020 5:52:35 PM","2020-09-15T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Mooring winch - Mooring winch #3 hydraulic oil leakage from valve block ","Deck - Mooring Machinery","Mooring","Equipment Related","11.4","Very High","","","Leakage rectified by replacing by sealing rings.","2020-09-30T23:59:35","","Completed","2020-10-28T23:59:35","No","No","No","Internal"]
[null,null,null,14213,null,"50_05/10/2020 5:57:03 PM","2020-09-15T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Mooring winch - Mooring winch foundation rusted ","Deck - Mooring Machinery","Mooring","External Factors","9.15","Medium","","","Derusting and painting completed","2020-12-10T23:59:35","","Completed","2020-12-01T23:59:35","No","No","No","Internal"]
[null,null,null,14214,null,"50_05/10/2020 5:58:41 PM","2020-09-15T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Mooring winch -Mooring winch # 6 brake band rusted - ","Deck - Mooring Machinery","Mooring","External Factors","9.15","Medium","","","Derusted and painted.","2020-10-15T23:59:35","","Completed","2020-10-15T23:59:35","No","No","No","Internal"]
[null,null,null,14216,null,"50_05/10/2020 6:06:07 PM","2020-09-15T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","COW - COW branch line to machines under side rusted – ","Deck - Pipe / Fittings","Cargo / Ballast Systems","External Factors","11.4","Very High","","","Maintenance in progress. Fresh observation raised.","2021-05-10T23:59:35","","Completed","2021-04-26T23:59:35","No","No","No","Internal"]
[null,null,null,14217,null,"50_05/10/2020 6:07:52 PM","2020-09-15T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Funnel - Funnel aft side stained ","Miscellaneous","General Appearance","External Factors","11.8","Low","","","Funnel aft side cleaned.","2020-10-10T23:59:35","","Completed","2020-10-03T23:59:35","No","No","No","Internal"]
[null,null,null,14218,null,"50_05/10/2020 6:00:20 PM","2020-09-15T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Deck pipeline - Main deck pipeline spot rusted","Deck - Pipe / Fittings","Cargo / Ballast Systems","External Factors","11.5","Medium","","","Maintenance in progress. Fresh observation raised.","2021-05-26T23:59:35","","Completed","2021-02-24T23:59:35","No","No","No","Internal"]
[null,null,null,14219,null,"50_05/10/2020 6:02:25 PM","2020-09-15T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Cargo System - Cargo System hydraulic valve box 2B wasted cover ","Deck - Pipe / Fittings","General Appearance","External Factors","11.3","Medium","","","Waster part of cover renewed.","2020-12-05T23:59:35","","Completed","2020-12-10T23:59:35","No","No","No","Internal"]
[null,null,null,14220,null,"50_05/10/2020 6:09:56 PM","2020-09-15T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Hose handling crane - Hose handling crane (STBD) hook noted not free ","Deck - Machinery","Cargo / Ballast Systems","Equipment Related","8.36","Medium","","","Freed up and fresh grease applied","2020-09-30T23:59:35","","Completed","2020-09-25T23:59:35","No","No","No","Internal"]
[null,null,null,14221,null,"50_05/10/2020 5:51:14 PM","2020-09-15T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Mooring winch - Mooring winch #2 hydraulic oil leakage from valve block ","Deck - Mooring Machinery","Mooring","Equipment Related","11.4","Very High","","","Leakage from operating lever rectified.","2020-09-30T23:59:35","","Completed","2020-09-26T23:59:35","No","No","No","Internal"]
[null,null,null,14222,null,"50_05/10/2020 6:04:47 PM","2020-09-15T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","SWL - Lifting lug outside P&S mid ship store SWL not marked ","Miscellaneous","General Appearance","Human Error","11.3","Medium","","","Lug Marked with SWL marking","2020-09-22T23:59:35","","Completed","2020-09-20T23:59:35","No","No","No","Internal"]
[null,null,null,14223,null,"50_05/10/2020 5:55:10 PM","2020-09-15T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Mooring winch - Mooring winch #6 hydraulic oil leakage from valve block ","Deck - Mooring Machinery","Mooring","Equipment Related","11.4","Very High","","","Hyd.oil leakage from operating lever rectified by renewing seal rings.","2020-09-30T23:59:35","","Completed","2020-09-30T23:59:35","No","No","No","Internal"]
[null,null,null,14225,null,"50_29/09/2020 3:56:19 PM","2020-09-16T23:59:35","Defect","Ship Staff","Ship Staff Insp.","1 Sheave Pillar for Stbd gangway swinging wire partially sheared off at base and bent.","Deck - Machinery","Structural Condn. / WT integrity ","Equipment Related","5.47","Medium","","","Temporary repairs and supports fitted by cold work - to carry out permanent repairs at next Dry Dock","2020-09-25T23:59:35","","Completed","2020-09-25T23:59:35","Yes","No","No","Internal"]
[null,null,null,16466,null,"50_04/01/2021 11:10:37","2020-09-23T23:59:35","Defect","Ship Staff","Ship Staff Insp.","SSAS transmitting actual alerts in test mode.\t","Elect. Mach. & Equip.,Miscellaneous","ISPS Related","Equipment Related","7.7","Low","","","Warstila technician communicated with the vessel's terminal remotely and re-programmed it. System tested on TEST mode and found working satisfactory.","2020-12-26T23:59:35","","Completed","2020-12-19T23:59:35","No","No","No","Internal"]
[null,null,null,14947,null,"50_15/11/2020 6:13:18 PM","2020-09-23T23:59:35","Critical Equipment,Defect","Ship Staff","Ship Staff Insp.","SSAS is transmitting actual Security Alert in Test Mode.","Critical Equip.","ISPS Related","Equipment Related","7.7","Low","","","Troubleshooring carried out as instrcted by Mr. kamlesh Solanki and SSAS technician. Defect rectified and SSAS working satisfactory.","2020-12-23T23:59:35","","Completed","2020-12-19T23:59:35","No","No","No","Internal"]
[null,null,null,14224,null,"50_03/10/2020 3:04:54 PM","2020-09-25T23:59:35","Defect","Ship Staff","Ship Staff Insp.","During routine inspection it was observed that the Hoisting wire for Port gangway has a lot of Broken strands and needs renewal.","Deck - Machinery","Safety / LSA / FFA","Equipment Related","5.47","Medium","","","Hoisting wire renewed using Spare wire on board.","2020-09-30T23:59:35","","Completed","2020-09-25T23:59:35","No","No","No","Internal"]
[null,null,null,16453,null,"50_04/01/2021 10:47:30","2020-11-11T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Pipe line leading to fuel oil drain tank are choked.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Main Pipe line renewed in 2021 drydock.","2021-03-11T23:59:35","","Completed","2021-02-26T23:59:35","No","No","No","Internal"]
[null,null,null,15576,null,"50_08/12/2020 20:26:36","2020-11-11T23:59:35","Non Conformity","Ship Staff","Ship Staff Insp.","Sewage treatment system discharge rate certificate to be endorsed by ABS surveyor","Documentation","Cert. & Docu.","Equipment Related","2.1","Very High","","","Discussed with ABS surveyor and as per him the certificate is valid with old class stamp. ABS verification is not required.","2021-03-11T23:59:35","","Completed","2021-03-01T23:59:35","No","No","No","Internal"]
[null,null,null,16454,null,"50_04/01/2021 10:37:12","2020-12-10T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Drain pipe from incinerator waste oil sett/serv tanks are choked with sludge. ","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Pipe line renewed in 2021 drydock.","2021-03-11T23:59:35","","Completed","2021-02-26T23:59:35","No","No","No","Internal"]
[null,null,null,16455,null,"50_04/01/2021 10:45:33","2020-12-10T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Drain pipes from purifier room are choke","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Drain pipes removed & cleaned. Drain cleared up.","2021-06-23T23:59:35","","Completed","2021-03-10T23:59:35","No","No","No","Internal"]
[null,null,null,16456,null,"50_04/01/2021 10:50:39","2020-12-10T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Aux boiler -2 remote level transmitter non functional","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Transmitter calibrated by service engineer in 2021 drydock. Now working satisfactory.","2021-03-11T23:59:35","","Completed","2021-02-26T23:59:35","No","No","No","Internal"]
[null,null,null,16457,null,"50_04/01/2021 10:53:25","2020-12-10T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Casing of various light fitting around accommodation and funnel corroded and holed.","Elect. Mach. & Equip.","Structural Condn. / WT integrity ","Equipment Related","11.11","Very High","","","All the corroded and damaged light fittings renewed.","2021-03-23T23:59:35","DPEO200216","Completed","2021-03-10T23:59:35","No","No","No","Internal"]
[null,null,null,16458,null,"50_04/01/2021 10:57:03","2020-12-10T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Digital readout panel for 5P, 3P and 2 HFO P is defective (no display)","Elect. Mach. & Equip.","Cargo / Ballast Systems","Equipment Related","8.8","Medium","","","NEw panels not available, same tried to procure during DD. As advised the system is redundant and secondary display. Primary display is operational and showing correct readings.","2021-03-10T23:59:35","DPEO200198","Completed","2021-02-28T23:59:35","No","No","No","Internal"]
[null,null,null,16459,null,"50_04/01/2021 10:59:23","2020-12-10T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Limit switch for port lifeboat crank handle storing stuck in activated condition.","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.29","High","","","Limit switch renewed and made functional.","2021-02-10T23:59:35","DPEO200217","Completed","2021-02-08T23:59:35","No","No","No","Internal"]
[null,null,null,13038,null,"50_07/07/2020 2:15:39 PM","2020-12-10T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","CCR – remote valve indicator- Few not matching with actual open/close Position","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.8","Medium","","","Adjusted and checked found working satisfactory.","2021-03-26T23:59:35","","Completed","2021-04-16T23:59:35","No","No","No","Internal"]
[null,null,null,15454,null,"50_07-Dec-20 5:49:38 PM","2020-12-11T23:59:35","Observation","Ship Staff","Ship Staff Insp.","M/E Performance checker DOCTOR unit not operational.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Pickup sensor renewed and performance recorded. Now working satisfactory.","2021-03-11T23:59:35","DPEO200210","Completed","2020-12-20T23:59:35","No","No","No","Internal",""]
[null,null,null,15577,null,"50_08/12/2020 20:43:42","2020-12-11T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Elevator calling button in B & C deck not operational. According to technician, sytem obsolate, no spares available.","Accommodation","MLC Related","Equipment Related","11.16","Low","","","PCBs for B & C deck renewed in 2021 dry dock by KUIDA technician. Now working satisfactory.","2021-03-11T23:59:35","","Completed","2021-02-27T23:59:35","No","No","No","Internal"]
[null,null,null,15578,null,"50_08/12/2020 20:32:00","2020-12-12T23:59:35","Observation","Ship Staff","Ship Staff Insp.","A/E #3, Additional Oil Max Filtering unit not yet installed.","E/R - Aux. Engine","Eng. / Strg. Comp.","External Factors","10.32","Very High","","","A/E #3 Oil max system installed and tested, found working satisfactory.","2021-03-12T23:59:35","DPEO205109","Completed","2021-03-16T23:59:35","No","No","No","Internal"]
[null,null,null,15579,null,"50_08/12/2020 20:36:43","2020-12-21T23:59:35","Defect","Ship Staff","Ship Staff Insp.","A/E #3 Unit no 7 suction valve actuator push rod bend, need to renew. Also Exh gas sensor not fitted as there is no spare.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","A/E #3 unit-7,  exhaust gas sensor renewed, now working satisfactory.","2021-03-23T23:59:35","DPEO205111 & DPEO200187","Completed","2021-02-28T23:59:35","No","No","No","Internal"]
[null,null,null,16460,null,"50_04/01/2021 11:01:29","2020-12-24T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","Aldis lamp battery discharged and not operational","Navigation - Others","Navigation","Equipment Related","4.7","High","","","New battery received and put in use. ALDIS lamp battery operatinal now.","2021-01-26T23:59:35","DPEO200242","Completed","2021-01-16T23:59:35","No","No","No","Internal"]
[null,null,null,16461,null,"50_04/01/2021 11:03:42","2020-12-25T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","Gauges on CCR panel for Bllast tank & bunker tank sounding and vessel's draft showing erratic values","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.8","Medium","","","Troubleshooting carried out by Kuida technician at Yiu Lian shipyard. Found 1 PCB is inoperational. As the remote gauges are secondary display, they will be discontinued. PRimary display and loadicator online readings are operational.","2021-03-02T23:59:35","","Completed","2021-02-28T23:59:35","No","No","No","Internal"]
[null,null,null,17492,null,"50_18/01/2021 8:46:23 AM","2020-12-25T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","D/G #2 fuel injection pump drain modified to loose container","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Main drain line renewed in dry dock and DG-2 section cleared. Loose container removed and drain pipe fitted normal to drain scupper.","2021-03-10T23:59:35","","Completed","2021-02-27T23:59:35","No","No","No","Internal"]
[null,null,null,17493,null,"50_18/01/2021 8:51:44 AM","2020-12-25T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Diesel Generator no. 1 fuel injection pump drain modified to loose container","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Main drain line renewed in dry dock and DG-1 section cleared. Loose container removed and drain pipe fitted normal to drain scupper.","2021-03-10T23:59:35","","Completed","2021-02-27T23:59:35","No","No","No","Internal"]
[null,null,null,17494,null,"50_17/01/2021 07:45:12","2020-12-25T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","DG-3 Exhaust pipe leakage ","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Various bellows and gaskets in the exhaust gas pipe renewed and leakages rectified in 2021 drydock. No further leakage observed during Engine operation.","2021-03-10T23:59:35","","Completed","2021-02-27T23:59:35","No","No","No","External"]
[null,null,null,17495,null,"50_18/01/2021 9:31:27 AM","2020-12-25T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ME exhaust pipe (after EGB) bellow leaking","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Bellow at C-deck level inspected found gasket damaged, same is renewed in drydock2021. No further leakage observed during engine operation.","2021-03-10T23:59:35","","Completed","2021-03-01T23:59:35","No","No","No","Internal"]
[null,null,null,17496,null,"50_18/01/2021 9:35:00 AM","2020-12-25T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ME exhaust pipe bellow (at boiler platform) leaking","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Exhaust pipe bellow renewed in 2021 drydock. No furher leakage during engine operation.","2021-03-23T23:59:35","","Completed","2021-02-27T23:59:35","No","No","No","Internal"]
[null,null,null,17497,null,"50_17/01/2021 11:25:47","2020-12-25T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Main engine exhaust bellow (2 nos) leakage","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.37","Medium","","","Bellow renewed at one location (2nd deck) and gasket renewed at 2nd location( Engine casing C-deck) in drydock 2021. No further leakage observed during engine operation.","2021-03-17T23:59:35","","Completed","2021-03-01T23:59:35","No","No","No","Internal"]
[null,null,null,17498,null,"50_17/01/2021 11:43:58","2020-12-25T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Oil leak form  pipe above ME jacket water pump","E/R - Pipes/ valves & fittings","MARPOL Related","Equipment Related","2.1","Very High","","","Oil leakge rectfied by reneweing the flange gasket. No further leakge observed. ","2021-03-19T23:59:35","","Completed","2021-01-15T23:59:35","No","No","No","Internal"]
[null,null,null,17534,null,"50_16/01/2021 11:36:45","2020-12-29T23:59:35","Observation","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","The ORB entry correction after wrong entry on 05 November 2020 in ORB part 1 and 10 March 2020 & 15 April 2020 in ORB part 2 were not dated by responsible officer required as per the guideline of ORB entry in MEPC/C 736 - This observation was rectified during this inspection.","Documentation","Cert. & Docu.","Human Error,Inappropriate Procedure","2.1","Very High","","","Date written against initials for all three corrections in ORB.Training of all officers carried out on correct entry and correction procedure. A poster attached to ORB describing procedure for corrections.","2021-02-23T23:59:35","","Completed","2020-12-29T23:59:35","No","No","No","External"]
[null,null,null,17535,null,"50_16/01/2021 11:38:49","2020-12-29T23:59:35","Observation","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","ALDIS lamp test with portable battery during inspection was found to be not satisfactory as battery was not fully charged.","Navigation - Others","Navigation","Equipment Related","4.7","High","","","ALDIS lamp battery was immediately put on charge and fully charged.Daily battery voltage check routine implemented. Onboard log made and posted near Aldis lamp battery storage area.","2021-02-23T23:59:35","","Completed","2020-12-31T23:59:35","No","No","No","External"]
[null,null,null,17536,null,"50_16/01/2021 11:40:53","2020-12-29T23:59:35","Observation","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","8 Nos x 17 litres and 15 Nos x 3 litres opened paint drums stored in paint store located exterior to accommodation deck were not secured with lashing at the time of inspection.","Miscellaneous","ISM Related","Behaviour Based","5.11","Low","","","Subjected paint drums were immediately lashed with rope lashing. Meeting carried out with all crew and importance of lashing paint drums and loose objects reiterated to all.","2021-02-23T23:59:35","","Completed","2020-12-29T23:59:35","No","No","No","External"]
[null,null,null,17537,null,"50_16/01/2021 11:42:59","2020-12-29T23:59:35","Observation","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","Records were available in shipboard PMS, but routine inspection record for the maintenance on various vent heads and flame screens fitted to ballast tanks, bunker tanks and void spaces did not identify the tanks individually.","Documentation,Hull & Tanks","Structural Condn. / WT integrity ","Inappropriate Procedure","11.7","High","","","Form edited to add inspection details of individual tank vent head and flame screen. Concerned officer familiarized with amended form. Office requested to add remark in the form “Details of individual tank to be added under each section to make the form ship specific”.","2021-02-23T23:59:35","","Completed","2020-12-31T23:59:35","No","No","No","External"]
[null,null,null,18194,null,"50_04/02/2021 6:34:42 PM","2021-01-26T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Port side life boat walk way grating support structure damage","LSA / FFA","Structural Condn. / WT integrity ","Equipment Related","11.1","High","","","New structure to fabricated and fitted.","2021-02-23T23:59:35","","Completed","2021-02-15T23:59:35","No","No","No","Internal"]
[null,null,null,24510,null,"50_23/03/2022 17:37:02","2021-02-16T23:59:35","Observation","Ship Staff","Suptd. Insp.","Incinerator draft fan motor and actuator not operating automatically. ","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Incinerator draft fan actuator renewed with newly received spares. Automatic operation confirmed. Incinerator tried out in sludge mode. All automatic opertation found to be working satisfactory.\n\n\n","2022-07-10T23:59:35","DPEO225039","Completed","2022-06-06T23:59:35","No","No","No","Internal"]
[null,null,null,18631,null,"50_14/03/2021 21:25:00","2021-03-03T23:59:35","Critical Equipment,Defect","Ship Staff","Ship Staff Insp.","SSAS transmitting actual alerts in test mode.","Miscellaneous","ISPS Related","Equipment Related","7.7","Low","","","New unit installed and cables laid, checked and found working satisfactorily.","2021-03-20T23:59:35","","Completed","2021-04-07T23:59:35","No","No","No","Internal"]
[null,null,null,16462,null,"50_04/01/2021 11:05:27","2021-03-05T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","Presure sensor for 4C COT not functioning, giving communication failure alarm.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.13","Medium","","","New TGU unit installed. Pressure sensor working satisfactory.","2021-09-25T23:59:35","DPEO210124","Completed","2021-09-24T23:59:35","No","No","No","Internal"]
[null,null,null,18632,null,"50_16/03/2021 13:07:07","2021-03-08T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Metal to metal contact on the Gangway wire guides.","Deck - Machinery","ISM Related","Inappropriate Procedure","5.47","Medium","","","Gangway shifting wire guide supports covered with PVC pipe to avoid wire directly coming in contact with guides.","2021-04-25T23:59:35","","Completed","2021-04-11T23:59:35","No","No","No","Internal"]
[null,null,null,18633,null,"50_16/03/2021 13:34:57","2021-03-08T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Improve upon the cosmetic condition of the Engine Room, Purifier room and Pump Room, specially lower ER platforms, pump-room bilges and stairways. ","Miscellaneous","ISM Related","Industry Issue","11.8","Low","","","Cosmetic condition of ER, Purifier room improved.","2021-04-25T23:59:35","","Completed","2021-04-25T23:59:35","No","No","No","Internal"]
[null,null,null,18647,null,"50_19/03/2021 10:06:49","2021-03-08T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Open bunker tank vent head","E/R - Pipes/ valves & fittings","Structural Condn. / WT integrity ","Behaviour Based","11.7","High","","","All the open bunker tank vent heads closed and fitted back","2021-06-08T23:59:35","","Completed","2021-03-08T23:59:35","No","No","No","Internal"]
[null,null,null,18648,null,"50_19/03/2021 10:09:53","2021-03-08T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","All loose hoses in E/R to secure","Miscellaneous","Eng. / Strg. Comp.","Behaviour Based","10.29","Medium","","","Loose hoses in E/R secured and stored in dedicated place in steering gear room.","2021-06-08T23:59:35","","Completed","2021-03-09T23:59:35","No","No","No","Internal"]
[null,null,null,18649,null,"50_19/03/2021 10:23:41","2021-03-08T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Missing railing at Main Engine manouvering plateform.","Miscellaneous","Eng. / Strg. Comp.","External Factors","10.29","Medium","","","Railing fitted back in place.","2021-06-08T23:59:35","","Completed","2021-03-10T23:59:35","No","No","No","Internal"]
[null,null,null,18650,null,"50_16/03/2021 09:41:55","2021-03-08T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Radar gauge remote display were not showing correct ullage","Elect. Mach. & Equip.","Cargo / Ballast Systems","Equipment Related","8.13","Medium","","","Radar gauge remote displays and Radar gauge system restarted. All remote displays for COT are operational now.","2021-04-10T23:59:35","","Completed","2021-03-13T23:59:35","No","No","No","Internal"]
[null,null,null,18651,null,"50_16/03/2021 13:03:02","2021-03-08T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Loose electrical cable in forecastle and have it removed / secured properly.","Elect. Mach. & Equip.","General Appearance","Human Error,Inappropriate Procedure","11.1","High","","","Old speed log tranducer cable cut and discarded.","2021-03-26T23:59:35","","Completed","2021-03-15T23:59:35","No","No","No","Internal"]
[null,null,null,18652,null,"50_16/03/2021 13:38:48","2021-03-08T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Hoses / Hydrant caps to be put back in place","LSA / FFA","Safety / LSA / FFA","Inappropriate Procedure","5.35","Medium","","","All hydrant caps put back in place.","2021-03-20T23:59:35","","Completed","2021-03-09T23:59:35","No","No","No","Internal"]
[null,null,null,18653,null,"50_16/03/2021 09:37:15","2021-03-08T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Hydraulic Leakages on 3 mooring winches to be rectified","Deck - Mooring Machinery","Mooring","Equipment Related","11.4","Very High","","","Leaking Mooring winch control block seals renewed and no leak obesrved during test operation.","2021-03-26T23:59:35","","Completed","2021-03-12T23:59:35","No","No","No","Internal"]
[null,null,null,18654,null,"50_19/03/2021 10:00:53","2021-03-08T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Oil leakages on steering gear system","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","oil leakages from steering gear ram cylinder end bolts rectified by inserting fabricated 5 mm copper washer. No further leakage observed.","2021-06-08T23:59:35","","Completed","2021-04-04T23:59:35","No","No","No","Internal"]
[null,null,null,18655,null,"50_16/03/2021 13:10:13","2021-03-08T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Cosmetic Upgrade of Mast riser main valve to be done","Deck - Pipe / Fittings","General Appearance","Inappropriate Procedure","11.4","Very High","","","Mast riser main valve painted with 1st & 2nd coat of primer followed by final coat.","2021-03-26T23:59:35","","Completed","2021-03-10T23:59:35","No","No","No","Internal"]
[null,null,null,18656,null,"50_16/03/2021 13:30:15","2021-03-08T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","All Stores need to be squared up","Miscellaneous","ISM Related","Industry Issue","11.12","Low","","","All stores arranged & squared up.","2021-03-26T23:59:35","","Completed","2021-03-26T23:59:35","No","No","No","Internal"]
[null,null,null,18660,null,"50_16/03/2021 13:26:03","2021-03-08T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","PV breaker tube to be cleaned so that level is clearly visible, graduation pipe to be marked with Normal level.","Inert Gas","Cargo / Ballast Systems","Equipment Related","8.28","Medium","","","Tube be cleaned. Procedure for checking correct water level is posted on the body of PV breaker. ","2021-03-26T23:59:35","","Completed","2021-03-13T23:59:35","No","No","No","Internal"]
[null,null,null,19386,null,"50_10/05/2021 07:28:14","2021-03-17T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Drain pipes from purifier room are choke","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Dismantled most of the pipelines from 3rd deck to 4th deck and cleared the pipelines and boxed back.","2021-06-23T23:59:35","","Completed","2021-05-20T23:59:35","No","No","No","Internal"]
[null,null,null,18657,null,"50_16/04/2021 02:48:14","2021-03-18T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Unable to operate 3C COT IG valve.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.19","High","","","Actuator inspected. Found roller bearing damaged. Replaced same with brass bush & boxed back. Defedt rectified.","2021-03-20T23:59:35","","Completed","2021-03-19T23:59:35","No","No","No","Internal"]
[null,null,null,18658,null,"50_15/04/2021 23:26:54","2021-03-19T23:59:35","Observation","Ship Staff","Ship Staff Insp.","BWTS system - Flow meter pipe found leaking.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.8","Medium","","","Flanges tightened up & leak rectified.","2021-03-19T23:59:35","","Completed","2021-03-19T23:59:35","No","No","No","Internal"]
[null,null,null,18659,null,"50_15/04/2021 23:29:30","2021-03-19T23:59:35","Observation","Ship Staff","Ship Staff Insp.","No. 1 WBP strainer lid found leaking.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.8","Medium","","","No. 1 WBP strainer lid tightened up. Leak rectified.","2021-03-20T23:59:35","","Completed","2021-03-20T23:59:35","No","No","No","Internal"]
[null,null,null,18661,null,"50_16/04/2021 02:54:57","2021-03-19T23:59:35","Defect","Ship Staff","Ship Staff Insp.","M1, M2, M3, M4, M5 & M6 winch dircetion control valves found leaking.","Deck - Mooring Machinery","Mooring","Equipment Related","9.14","Medium","","","Inspection carried out, DCV dismantled. Found step seals missing. Step seals placed & DCV boxed back. Winches tried out & no leak observed. ","2021-03-21T23:59:35","","Completed","2021-03-21T23:59:35","No","No","No","Internal"]
[null,null,null,18634,null,"50_16/04/2021 07:14:26","2021-03-20T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Leakage observed in FW line on deck.","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","Equipment Related","","","","","Gaskets from several flanges renewed to rectify leakages (20 flanges). 2 pcs of wasted sections of pipelies repaired.Leak from remaining 30 flanges rectified after receiving spares. System tried out satisfactorily.","2021-07-25T23:59:35","DPEO210080","Completed","2021-07-17T23:59:35","No","No","No","Internal"]
[null,null,null,18635,null,"50_16/04/2021 03:04:55","2021-03-23T23:59:35","Defect","Ship Staff","Ship Staff Insp.","2 sets of UTIS were found with wiper cover not properly fitted due to damaged locking arrangement, leading to seepage of oil while heaving up UTI.","Miscellaneous","Cargo / Ballast Systems","Equipment Related","8.12","Medium","","","Office notified. Vessel will off-land same for repairs at the next opportunity.\n\nService technicians attended both UTIs onboard at Singapore on 8th July 2021. Both UTIs tried out & found working satisfactorily.\n\n","2021-07-03T23:59:35","DPEO215102","Completed","2021-07-04T23:59:35","No","No","No","Internal"]
[null,null,null,18662,null,"50_16/04/2021 06:52:19","2021-03-27T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Port bridge wing search light found without any locking arrangement for setting angle.","Miscellaneous","Safety / LSA / FFA","Equipment Related","5.47","Medium","","","New locking arrangement fabricated.","2021-04-25T23:59:35","","Completed","2021-03-29T23:59:35","No","No","No","Internal"]
[null,null,null,18663,null,"50_16/04/2021 07:53:55","2021-03-28T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Several WBT sounding pipes found with caps not closing properly.","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","Equipment Related","11.7","High","","","All caps & sounding pipes thread cleaned up & repaired. Greasing carried out & defect rectified.","2021-04-05T23:59:35","","Completed","2021-03-30T23:59:35","No","No","No","Internal"]
[null,null,null,18664,null,"50_16/04/2021 06:58:08","2021-03-30T23:59:35","Observation","Ship Staff","Ship Staff Insp.","No. 2 WBP casing found leaking from joint.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.8","Medium","","","Casing tightened up. Leak rectified.","2021-03-31T23:59:35","","Completed","2021-03-30T23:59:35","No","No","No","Internal"]
[null,null,null,18944,null,"50_30/04/2021 18:59:16","2021-03-31T23:59:35","Observation","Ship Staff","Ship Staff Insp.","M1 & M5 winch control levers found jammed & difficult to operate.","Deck - Mooring Machinery","Mooring","Equipment Related","9.14","Medium","","","Both brake control blocks removed, O rings renewed & levers freed up.","2021-04-02T23:59:35","","Completed","2021-04-02T23:59:35","No","No","No","Internal"]
[null,null,null,18945,null,"50_30/04/2021 07:34:32","2021-04-01T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Deck seal overboard line found clogged as deck seal water level found risng & not draining at required rate.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Industry Issue","8.27","Medium","","","Deck seal pump stopped. Section of overboard line opened up on deck. Overboard line blown through & clogging removed.","2021-04-10T23:59:35","","Completed","2021-04-02T23:59:35","No","No","No","Internal"]
[null,null,null,18946,null,"50_30/04/2021 07:56:04","2021-04-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","No. 4 manifold pressure gauge (Port side) found defective with steady pressure reading of 1.5 bar.","Miscellaneous","Cargo / Ballast Systems","Equipment Related","8.41","Medium","","","Pressure gauge renewed.","2021-04-02T23:59:35","","Completed","2021-04-02T23:59:35","No","No","No","Internal"]
[null,null,null,18947,null,"50_30/04/2021 19:13:33","2021-04-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Aft ETA operating lever locking pin found wasted.","Miscellaneous","Emgcy. Systems","Equipment Related","9.29","Low","","","New locking pin fabricated & fixed back.","2021-04-03T23:59:35","","Completed","2021-04-03T23:59:35","No","No","No","Internal"]
[null,null,null,19571,null,"50_30/05/2021 08:19:59","2021-04-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Stripper pump strainer lid found leaking.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.8","Medium","","","Lid opened up for inspection. Rubberpacking found damaged. New Gasket installed & leak arrested.","2021-05-26T23:59:35","","Completed","2021-05-17T23:59:35","No","No","No","Internal"]
[null,null,null,18636,null,"50_16/04/2021 03:17:32","2021-04-02T23:59:35","Defect","Ship Staff","Ship Staff Insp.","WBT 4P (Aft). WBT 4S (Aft). & WBT 5P (Aft). gas sampling flow fault. ","Miscellaneous","Safety / LSA / FFA","Equipment Related","5.21","Medium","","","All 3 sampling lines interchanged to use with known good solenoids & no alarm observed.Solenoids of these 3 tanks interchanged to use with known good sampling lines, still flow fault alarm occurred. Flame arrestors found chocked, same cleaned & placed back. Flow fault rectified.","2021-05-25T23:59:35","","Completed","2021-05-03T23:59:35","No","No","No","Internal"]
[null,null,null,18637,null,"50_16/04/2021 03:22:35","2021-04-02T23:59:35","Observation","Ship Staff","Ship Staff Insp.","WBT 2P (Aft) & WBT 2S (Aft) gas sampling flow fault. ","Miscellaneous","Safety / LSA / FFA","Equipment Related","5.21","Medium","","","Solenoids observed working satisfactorily. Lines blown through & filter cleaned. System tried out. 2P (Aft) flow fault rectified completely. 2S (Aft) rectified, however, same reoccured after 2 days. Rectification in progress. 03-May-2021: 2S Aft attended again, lines blown through, filter cleaned. System connected & flow fault rectified.","2021-05-10T23:59:35","","Completed","2021-04-28T23:59:35","No","No","No","Internal"]
[null,null,null,18638,null,"50_16/04/2021 11:38:31 PM","2021-04-02T23:59:35","Observation","Ship Staff","Engineering Audit","M/E Load indicator showing fault ","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Renewed the linkage","2021-09-25T23:59:35","DPEO210074","Completed","2021-09-24T23:59:35","No","No","No","Internal"]
[null,null,null,18639,null,"50_16/04/2021 11:45:52 PM","2021-04-02T23:59:35","Defect","Ship Staff","Engineering Audit","Leakage observed in Air system for Blower flaps","Miscellaneous","Safety / LSA / FFA","Equipment Related","10.18","High","","","All connections checked and tightened as required, new ferrule connections made and leakage rectified.","2021-07-02T23:59:35","DPEO210075","Completed","2021-04-18T23:59:35","No","No","No","Internal"]
[null,null,null,18640,null,"50_16/04/2021 11:51:14 PM","2021-04-02T23:59:35","Defect","Ship Staff","Engineering Audit","M/E local thermometer pockets missing for units no.s 5 & 7","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Landed ashore at singapore for correct size, awaiting supply of the same.","2023-08-29T23:59:35","ITEM NO. 23 DPEO220026","Completed","2023-07-19T23:59:35","No","No","No","Internal","Twice quotes was sent to vsl - but specs not matching.\nchecking with vendors in China."]
[null,null,null,18641,null,"50_16/04/2021 11:56:33 PM","2021-04-02T23:59:35","Defect","Ship Staff","Engineering Audit","Waste gate for Turbocharger not in operation","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Fitted the waste gate in place, need to caliberate","2021-09-25T23:59:35","DPEO215117","Completed","2021-09-25T23:59:35","No","No","No","Internal"]
[null,null,null,18642,null,"50_17/04/2021 12:01:34 AM","2021-04-02T23:59:35","Defect","Ship Staff","Engineering Audit","EGB Soot blowers motors tripping on overload.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Eased up the soot blowers mechanically and modified the circuit in the control panel. Presently operational by push button.","2021-07-02T23:59:35","","Completed","2021-04-15T23:59:35","No","No","No","Internal"]
[null,null,null,18643,null,"50_17/04/2021 12:03:36 AM","2021-04-02T23:59:35","Defect","Ship Staff","Engineering Audit","No.1 Reefer compressor Ammeter missing","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Renewed ammeter from spare and tried out found working satisfactorily.","2021-07-02T23:59:35","","Completed","2021-04-21T23:59:35","No","No","No","Internal"]
[null,null,null,18644,null,"50_17/04/2021 12:06:36 AM","2021-04-02T23:59:35","Defect","Ship Staff","Engineering Audit","Sewage holding tank level gauge not in operation.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Found the float stuck same eased up and checked found working satisfactorily.","2021-07-02T23:59:35","","Completed","2021-04-15T23:59:35","No","No","No","Internal"]
[null,null,null,18645,null,"50_17/04/2021 12:08:58 AM","2021-04-02T23:59:35","Observation","Ship Staff","Engineering Audit","Auxiliary boiler diesel oil line filter missing","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","Spare Filter found in store removed, cleaned and boxed back.","2021-07-02T23:59:35","","Completed","2021-05-08T23:59:35","No","No","No","Internal"]
[null,null,null,18948,null,"50_30/04/2021 21:09:11","2021-04-06T23:59:35","Defect","Ship Staff","Ship Staff Insp.","One of the sprinkler head of port side life boat found damaged.","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","New sprinkler head fabricated & fitted.","2021-04-07T23:59:35","","Completed","2021-04-07T23:59:35","No","No","No","Internal"]
[null,null,null,18949,null,"50_30/04/2021 21:41:58","2021-04-06T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Stbd. lifeboat sprinkler valve found not holding.","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.29","High","","","Sprinkler valve inspected. Position of control lever was obscured by battery selector switch to close properly. Position of valve contrl lever adjusted to make valve completely shut.","2021-04-25T23:59:35","","Completed","2021-04-19T23:59:35","No","No","No","Internal"]
[null,null,null,18950,null,"50_30/04/2021 21:11:23","2021-04-07T23:59:35","Defect","Ship Staff","Ship Staff Insp.","3 pcs of fixed chairs in crew mes room were found damaged.","Accommodation","General Appearance","Equipment Related","","","","","Repairs carried out on chairs.","2021-04-08T23:59:35","","Completed","2021-04-08T23:59:35","No","No","No","Internal"]
[null,null,null,18951,null,"50_30/04/2021 21:17:15","2021-04-08T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Several chain blocks were found with loose & missing safety latches","Miscellaneous","ISM Related","Equipment Related","","","","","Safety latches installed for missin ones & springs renewed for loose ones","2021-04-09T23:59:35","","Completed","2021-04-08T23:59:35","No","No","No","Internal"]
[null,null,null,18952,null,"50_30/04/2021 21:22:09","2021-04-08T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Pumproom davit hook safety latch found missing.","Miscellaneous","ISM Related","Equipment Related","2.3","High","","","New safety latch fabricated & installed.","2021-04-11T23:59:35","","Completed","2021-04-11T23:59:35","No","No","No","Internal"]
[null,null,null,18953,null,"50_30/04/2021 21:27:35","2021-04-09T23:59:35","Defect","Ship Staff","Ship Staff Insp.","A deck port side door emergency unlocking arrangement found damaged.","Accommodation","ISPS Related","Equipment Related","","","","","Unlocking arrangement repaired & defect rectified.","2021-04-11T23:59:35","","Completed","2021-04-11T23:59:35","No","No","No","Internal"]
[null,null,null,18959,null,"50_30/04/2021 21:06:58","2021-04-10T23:59:35","Defect","Ship Staff","Ship Staff Insp.","No. 2 foam monitor valve found leaking","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.4","High","","","No. 2 foam monitor valve renewed. Leak rectified.","2021-04-12T23:59:35","","Completed","2021-04-12T23:59:35","No","No","No","Internal"]
[null,null,null,18954,null,"50_30/04/2021 21:35:48","2021-04-12T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Both pumproom blower fire dampers found inoperational.","Miscellaneous","Emgcy. Systems","Equipment Related","5.19","Medium","","","Both pump room blower damper control valves found inoperational. New set of arrangement installed & tried out to be working satisfactory.","2021-04-16T23:59:35","","Completed","2021-04-16T23:59:35","No","No","No","Internal"]
[null,null,null,18955,null,"50_30/04/2021 21:44:40","2021-04-12T23:59:35","Defect","Ship Staff","Ship Staff Insp.","W1-B brake control lever found damaged.","Deck - Mooring Machinery","Mooring","Equipment Related","9.14","Medium","","","Brake control block removed. Broken lever removed & new lever installed.","2021-04-25T23:59:35","","Completed","2021-04-14T23:59:35","No","No","No","Internal"]
[null,null,null,18956,null,"50_30/04/2021 22:20:15","2021-04-12T23:59:35","Defect","Ship Staff","Ship Staff Insp.","No. 2 foam monitor platform securing chains detached from the platform bar due to damaged securing eye.","Miscellaneous","ISM Related","Equipment Related","","","","","Damaged securing eye removed & new securing eye fabricated & installed.","2021-04-25T23:59:35","","Completed","2021-04-18T23:59:35","No","No","No","Internal"]
[null,null,null,18957,null,"50_30/04/2021 21:51:25","2021-04-15T23:59:35","Defect","Ship Staff","Ship Staff Insp.","M5 winch return hydraulic line found wasted & leaking.","Deck - Mooring Machinery","Mooring","Equipment Related","9.14","Medium","","","Line removed, repaired & installed back. Winch tried out without any leak.","2021-04-17T23:59:35","","Completed","2021-04-17T23:59:35","No","No","No","Internal"]
[null,null,null,18958,null,"50_30/04/2021 21:57:03","2021-04-16T23:59:35","Defect","Ship Staff","Ship Staff Insp.","M3 winch brake upper band damaged during BHC test.","Deck - Mooring Machinery","Mooring","Equipment Related","9.14","Medium","","","Band end was thinned down & got damaged during brake test. Same renewed with new one. BHC test caried out satisfactorily.","2021-04-16T23:59:35","","Completed","2021-04-16T23:59:35","No","No","No","Internal"]
[null,null,null,18942,null,"50_30/04/2021 07:28:20","2021-04-18T23:59:35","Defect","Ship Staff","Ship Staff Insp.","M7 mooring winch direction control valve found leaking from base.","Deck - Mooring Machinery","Mooring","Equipment Related","9.14","Medium","","","DCV block removed, found O ring flattend up. Same replaced with new one & leak rectified. After few operation. Leak occured again. DCV block removed, O ring placed back with silicone. Leak rectified. System tried out.","2021-05-26T23:59:35","","Completed","2021-05-09T23:59:35","No","No","No","Internal"]
[null,null,null,19434,null,"50_11/05/2021 19:04:03","2021-04-20T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Stbd. lifeboat embarkation deck light post wing nut missing\t","Deck - Pipe / Fittings","Safety / LSA / FFA","External Factors","5.29","High","","","New wing nut fabricated & fixed","2021-05-10T23:59:35","","Completed","2021-04-21T23:59:35","No","No","No","Internal"]
[null,null,null,19435,null,"50_11/05/2021 19:42:26","2021-04-20T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Stbd. side wilden pump discharge hose which is connected to a valve on top of Slop stbd. manhole was found damaged.","Deck - Pipe / Fittings,Miscellaneous","MARPOL Related","External Factors","6.3","Low","","","Damaged hose replaced with new one. Valve on top of slop stbd. manhole fitted with an elbow extension pipe to ensure orientation of fitting of wilden pump discharge hose is horizontal which will prevent bending & further damage. Same carried out for slop port tank.","2021-05-10T23:59:35","","Completed","2021-04-22T23:59:35","No","No","No","Internal"]
[null,null,null,19436,null,"50_11/05/2021 19:46:34","2021-04-20T23:59:35","Non Conformity","Ship Staff","Ship Staff Insp.","One of the foam extinguisher was obscured by BWTS electrolysis unit on engine room 2nd deck.","LSA / FFA","Safety / LSA / FFA","Behaviour Based","","","","","Fire extinguisher stowed to nearby location & all crew notified. No amendment in fire plan required as same is shifted to very close by location and by observing the fire plan, this extinguisher can be located.","2021-05-10T23:59:35","","Completed","2021-04-24T23:59:35","No","No","No","Internal"]
[null,null,null,19437,null,"50_11/05/2021 17:51:45","2021-04-25T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Stbd. bridge wing pneumatic service line valve found leaking.","Deck - Pipe / Fittings","General Appearance","External Factors","11.4","Very High","","","Valve renewed.","2021-05-10T23:59:35","","Completed","2021-04-26T23:59:35","No","No","No","Internal"]
[null,null,null,19442,null,"50_11/05/2021 20:01:28","2021-04-25T23:59:35","Defect","Ship Staff","Ship Staff Insp.","M5 winch return hydraulic line found wasted & leaking.","Deck - Mooring Machinery","Mooring","Equipment Related","","","","","Line removed, repaired & installed back. Winch tried out without any leak.","2021-04-28T23:59:35","","Completed","2021-04-28T23:59:35","No","No","No","Internal"]
[null,null,null,18943,null,"50_30/04/2021 16:09:26","2021-04-25T23:59:35","Defect","Ship Staff","Ship Staff Insp.","One of the  GMDSS Survival radio Speaker unit found in-operative.","LSA / FFA","Communication","Equipment Related","4.27","High","","","trouble shooting carried out as per manufacturer instructions and found TX,RX and Microphone unit in normal working order only the speaker unit is in-operative.\n\n\n\n\n\n\n\nI.E., We can not hear any transmission that is received by this radio (Speaker inoperational) & transmission made through this radio can be heard on other Radio(s) (Microphone operational). New radio received & tried out.","2021-05-25T23:59:35","DPEO215095","Completed","2021-06-01T23:59:35","No","No","No","Internal"]
[null,null,null,19322,null,"50_01/05/2021 19:21:28","2021-04-26T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Main deck Pipe U bolts - Few bolts found rusted.","Deck - Pipe / Fittings","General Appearance","External Factors","11.5","Medium","","","Derusting & painting carried out.","2021-07-26T23:59:35","","Completed","2021-05-03T23:59:35","No","No","No","Internal"]
[null,null,null,19323,null,"50_01/05/2021 20:59:23","2021-04-26T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Deck outfittings - At various stages of corrosion","Deck - Pipe / Fittings","General Appearance","External Factors","11.3","Medium","","","Derusting & painting carried out.","2021-07-26T23:59:35","","Completed","2021-04-26T23:59:35","No","No","No","Internal"]
[null,null,null,19324,null,"50_01/05/2021 21:02:14","2021-04-26T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Main deck - Cable tray running parallel to cargo pipes at various stages of corrosion.","Deck - Pipe / Fittings","General Appearance","External Factors","11.5","Medium","","","Derusting & painting carried out","2021-07-26T23:59:35","","Completed","2021-04-28T23:59:35","No","No","No","Internal"]
[null,null,null,19325,null,"50_01/05/2021 21:04:49","2021-04-26T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","COW - COW branch lines to machine underside rusted.","Deck - Pipe / Fittings","Cargo / Ballast Systems","External Factors","11.4","Very High","","","Derusting & painting carried out.","2021-07-26T23:59:35","","Completed","2021-04-30T23:59:35","No","No","No","Internal"]
[null,null,null,19326,null,"50_01/05/2021 21:07:31","2021-04-26T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Deck pipeline - Main deck pipelines spot rusted","Deck - Pipe / Fittings","Cargo / Ballast Systems","External Factors","11.5","Medium","","","Derusting & painting carried out.","2021-07-26T23:59:35","","Completed","2021-05-02T23:59:35","No","No","No","Internal"]
[null,null,null,19438,null,"50_11/05/2021 18:11:38","2021-04-26T23:59:35","Observation","Ship Staff","Ship Staff Insp.","2 pcs. of safety walkway wires on deck found in poor condition with eye almost damaged.","Miscellaneous","Safety / LSA / FFA","External Factors","5.47","Medium","","","Wires replaced with new one.","2021-05-10T23:59:35","","Completed","2021-05-08T23:59:35","No","No","No","Internal"]
[null,null,null,19439,null,"50_11/05/2021 20:15:03","2021-04-28T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Pumproom rescue davit slewing motor collar found damaged & seized due to oxidation (Aluminium collar)","Deck - Machinery","Emgcy. Systems","Equipment Related","8.5","Very High","","","Seized collar removed along with slewing motor. Spare motor overhauled & replaced damaged collar motor.","2021-05-10T23:59:35","","Completed","2021-04-29T23:59:35","No","No","No","Internal"]
[null,null,null,19440,null,"50_11/05/2021 20:19:06","2021-04-29T23:59:35","Defect","Ship Staff","Ship Staff Insp.","A pk tank & 4S WBT vent head covers found damaged while inspection & derusting.","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","External Factors","11.7","High","","","Both covers repaired, painted & boxed back.","2021-05-10T23:59:35","","Completed","2021-04-29T23:59:35","No","No","No","Internal"]
[null,null,null,19441,null,"50_11/05/2021 20:07:12","2021-04-29T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Stbd. wilden pump discharege valve connected to slop stbd. manhole found leaking.","Deck - Pipe / Fittings","MARPOL Related","External Factors","6.3","Low","","","Valve removed for overhauling. Condition of seat found beyond repairs. New valve installed.","2021-05-10T23:59:35","","Completed","2021-05-01T23:59:35","No","No","No","Internal"]
[null,null,null,19443,null,"50_11/05/2021 20:27:33","2021-04-29T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Stbd. provision crane hook safety latch spring found damaged.","Deck - Machinery","Safety / LSA / FFA","Equipment Related","8.5","Very High","","","New spring installed.","2021-05-10T23:59:35","","Completed","2021-04-30T23:59:35","No","No","No","Internal"]
[null,null,null,19444,null,"50_11/05/2021 20:36:25","2021-04-30T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Accommodation bulkhead fire plan container clamps found damaged.","LSA / FFA","Safety / LSA / FFA","External Factors","5.37","Low","","","New clamps fabricated for both side fire plans. Fire plan container installed with new clamps.","2021-05-10T23:59:35","","Completed","2021-05-03T23:59:35","No","No","No","Internal"]
[null,null,null,19445,null,"50_15/05/2021 17:09:56","2021-05-05T23:59:35","Defect","Ship Staff","Ship Staff Insp.","PV breaker gauge glass found cracked & supporting angle bar found corroded / wasted.","Deck - Pipe / Fittings","Cargo / Ballast Systems","External Factors","8.28","Medium","","","Gauge glass renewed / Supporting angle bar fabricated & renewed.","2021-05-05T23:59:35","","Completed","2021-05-08T23:59:35","No","No","No","Internal"]
[null,null,null,19566,null,"50_30/05/2021 16:56:24","2021-05-06T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Galley - Dough maker found not inoperational.","Miscellaneous","MLC Related","Equipment Related","","","","","Motor side inspected & found satisfactory. All Gears inspectd, overhauled & regreased. 2 pcs of bearings found not rotating freely. Both renewed.","2021-08-05T23:59:35","","Completed","2021-06-22T23:59:35","No","No","No","Internal"]
[null,null,null,19446,null,"50_15/05/2021 19:41:23","2021-05-06T23:59:35","Defect","Ship Staff","Ship Staff Insp.","2S & 3S WBT vent head covers found damaged while inspection & derusting.","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","External Factors","11.7","High","","","Both covers repaired, painted & boxed back.","2021-05-10T23:59:35","","Completed","2021-05-06T23:59:35","No","No","No","Internal"]
[null,null,null,19447,null,"50_15/05/2021 19:47:19","2021-05-06T23:59:35","Non Conformity","Ship Staff","Ship Staff Insp.","Mast riser fire fighting system – Steam supply valve spindle found broken.","Deck - Pipe / Fittings","Safety / LSA / FFA","External Factors","5.4","High","","","Valve renewd","2021-05-07T23:59:35","","Completed","2021-05-07T23:59:35","No","No","No","Internal"]
[null,null,null,19433,null,"50_15/05/2021 15:36:58","2021-05-07T23:59:35","Observation","Ship Staff","Ship Staff Insp.","WBT 4S (Aft) WBT gas sampling flow fault.","Miscellaneous","Safety / LSA / FFA","Equipment Related","5.21","Medium","","","Lines disconnected & blown through. Filters cleaned. Alarm still persists with disconnected lines. Solenoid found heating up slightly. Suspecting issue with opening of solenoid valve for 4S aft sampling. Solenoid valve cleaned up & flow fault rectified.","2021-05-26T23:59:35","","Completed","2021-05-22T23:59:35","No","No","No","Internal"]
[null,null,null,19572,null,"50_30/05/2021 08:08:36","2021-05-08T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Height of dump valve spindles shorter than height of adjacent fish plate.","Deck - Pipe / Fittings","MARPOL Related","Behaviour Based","6.3","Low","","","All dump valve spindles extended so that they can be located & operated in case of oil spill up to the level of fish plate.","2021-05-26T23:59:35","","Completed","2021-05-20T23:59:35","No","No","No","Internal"]
[null,null,null,19448,null,"50_15/05/2021 19:49:49","2021-05-08T23:59:35","Defect","Ship Staff","Ship Staff Insp.","1S WBT vent head body found wasted & holed.","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","External Factors","11.7","High","","","Vent head removed. Repaired in workshop & fixed back.","2021-05-10T23:59:35","","Completed","2021-05-09T23:59:35","No","No","No","Internal"]
[null,null,null,19449,null,"50_15/05/2021 19:55:32","2021-05-08T23:59:35","Defect","Ship Staff","Ship Staff Insp.","F. pk store natural vent flap - One piece of butterfly bolt found broken","Miscellaneous","Structural Condn. / WT integrity ","External Factors","11.6","Medium","","","New butterfly bolt fabricated & renewed","2021-05-26T23:59:35","","Completed","2021-05-10T23:59:35","No","No","No","Internal"]
[null,null,null,19432,null,"50_15/05/2021 16:57:37","2021-05-09T23:59:35","Defect","Ship Staff","Ship Staff Insp.","one of the GX 2009 personal gas meter could not be switched on.\n\nThis meter will only start when it is charging, and turns off as soon as it is removed from charger.","Miscellaneous","Safety / LSA / FFA","Equipment Related","5.23","Very High","","","Contractor 'The Bruusguaard system' infromed for troubleshooting advise. New gas meter will be supplied at Singapore.\n\nNew unit received at Singapore on 8th July 2021.\n\n","2021-07-10T23:59:35","DPEO215098","Completed","2021-07-03T23:59:35","No","No","No","Internal"]
[null,null,null,19450,null,"50_15/05/2021 19:52:45","2021-05-09T23:59:35","Defect","Ship Staff","Ship Staff Insp.","M1 winch fwd - Upper brake band found damaged with spindle bent.","Deck - Mooring Machinery","Mooring","Equipment Related","9.14","Medium","","","M1 winch fwd - Upper band renewed with new one. Spindle renewed.","2021-05-10T23:59:35","","Completed","2021-05-09T23:59:35","No","No","No","Internal"]
[null,null,null,19573,null,"50_30/05/2021 07:50:14","2021-05-11T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Paint store sprinkler system - One of the sprinkler head found detached from the pipe due to worn out threads of the sprinkler head & supply pipe. One more sprinkler head fount attached to the pipe but with damaged threads on pipe.","LSA / FFA","Safety / LSA / FFA","External Factors","5.35","Medium","","","Sprinkler head threads repaired. Sprinkler pipes removed, 2 pcs. of coupling repaired. All boxed back.","2021-05-25T23:59:35","","Completed","2021-05-12T23:59:35","No","No","No","Internal"]
[null,null,null,19574,null,"50_30/05/2021 16:41:34","2021-05-14T23:59:35","Defect","Ship Staff","Ship Staff Insp.","No. 1 hydraulic box cover found wasted at several places.","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","External Factors","11.5","Medium","","","Cover removed & repairs carried out.","2021-05-26T23:59:35","","Completed","2021-05-24T23:59:35","No","No","No","Internal"]
[null,null,null,19565,null,"50_30/05/2021 07:30:32","2021-05-15T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Stbd. provision crane -  Body of slewing motor found wasted  at several locations.","Deck - Machinery","Structural Condn. / WT integrity ","Equipment Related","8.5","Very High","","","All 3 leaking plugs renewed. Leak rectified.","2021-07-25T23:59:35","","Completed","2021-05-15T23:59:35","No","No","No","Internal"]
[null,null,null,19575,null,"50_30/05/2021 08:14:10","2021-05-15T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Stbd. provision crane - slewing motor hydraulic block found leaking from 3 locations.","Deck - Machinery","Structural Condn. / WT integrity ","Equipment Related","8.5","Very High","","","All 3 leaking plugs renewed. Leak rectified.","2021-05-26T23:59:35","","Completed","2021-05-15T23:59:35","No","No","No","Internal"]
[null,null,null,19576,null,"50_30/05/2021 08:28:52","2021-05-17T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Port & stbd. inboard dump valve spindles found free to rotate as connecting rods were found disconnected & making inboard dump valve inoperational.","Deck - Pipe / Fittings","MARPOL Related","Equipment Related","6.3","Low","","","Both inboard dump valve connecting rods connected back.","2021-05-26T23:59:35","","Completed","2021-05-19T23:59:35","No","No","No","Internal"]
[null,null,null,19577,null,"50_30/05/2021 08:25:28","2021-05-18T23:59:35","Observation","Ship Staff","Ship Staff Insp.","3C vacuum valve found leaking.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.19","High","","","Spare vacuum valve for center tanks overhauled. Replaced with 3C vacuum valve & leak arrested. 3C vacuum valve overhauled & kept as spare.","2021-05-26T23:59:35","","Completed","2021-05-24T23:59:35","No","No","No","Internal"]
[null,null,null,19567,null,"50_30/05/2021 16:59:11","2021-05-19T23:59:35","Defect","Ship Staff","Ship Staff Insp.","M6 mooring winch brake cylinder found leaking.","Deck - Mooring Machinery","Mooring","Equipment Related","9.14","Medium","","","Renewed the seals tried out working satisfactory","2021-08-10T23:59:35","","Completed","2021-07-31T23:59:35","No","No","No","Internal"]
[null,null,null,19569,null,"50_30/05/2021 16:50:55","2021-05-19T23:59:35","Observation","Ship Staff","Ship Staff Insp.","One of the hydraulic supply line flage in F. Pk. store found leaking.","Deck - Machinery","Mooring","External Factors","9.14","Medium","","","Flange's nuts and bolts tightened. Leak stopped. Confirmed by operation of winches.","2021-08-10T23:59:35","","Completed","2021-09-01T23:59:35","No","No","No","Internal"]
[null,null,null,19578,null,"50_30/05/2021 16:24:19","2021-05-19T23:59:35","Observation","Ship Staff","Ship Staff Insp.","2 pcs. of whels missing from WBP vent valves.","Cargo Mach.","Cargo / Ballast Systems","Human Error","8.8","Medium","","","Missing whels fixed back.","2021-05-26T23:59:35","","Completed","2021-05-22T23:59:35","No","No","No","Internal"]
[null,null,null,19579,null,"50_30/05/2021 16:36:43","2021-05-19T23:59:35","Defect","Ship Staff","Ship Staff Insp.","1P & 2P WBT vent head covers found damaged while inspection & derusting.","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","External Factors","11.7","High","","","Both covers repaired, painted & boxed back.","2021-05-26T23:59:35","","Completed","2021-05-22T23:59:35","No","No","No","Internal"]
[null,null,null,19568,null,"50_30/05/2021 16:33:43","2021-05-23T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Stbd. lifeboat air bottle manifold block is suspected to be leaking.","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.29","High","","","Need to dismantle all fitting enclosing air bottles to access the manifold block, to identify & rectify the leak. Some of the gaskets found missing. Leak rectified by placing new gaskets in the hose manifold block.","2021-06-02T23:59:35"," ","Completed","2021-05-26T23:59:35","No","No","No","Internal"]
[null,null,null,19580,null,"50_30/05/2021 16:30:18","2021-05-23T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Port lifeboat - Air supply valve coupling before pressure regulator valve found leaking.","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.29","High","","","Leak rectified from coupling.","2021-06-02T23:59:35","","Completed","2021-05-23T23:59:35","No","No","No","Internal"]
[null,null,null,19570,null,"50_30/05/2021 16:46:31","2021-05-24T23:59:35","Defect","Ship Staff","Ship Staff Insp.","F. pk store natural vent louver & cover found damaged.","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","External Factors","11.6","Medium","","","Louver & cover removed. Repaired in workshop. Painted & boxed back.","2021-06-10T23:59:35","","Completed","2021-06-06T23:59:35","No","No","No","Internal"]
[null,null,null,19714,null,"50_16/06/2021 07:33:49","2021-05-26T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Stbd. provision crane winch limit switch not operational.","Deck - Machinery","Cargo / Ballast Systems","Human Error","8.5","Very High","","","Limit switch adjusted to be operated.","2021-06-25T23:59:35","","Completed","2021-05-27T23:59:35","No","No","No","Internal"]
[null,null,null,19715,null,"50_16/06/2021 17:19:49","2021-05-26T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Port provision crane winch limit switch not operational.","Deck - Machinery","Cargo / Ballast Systems","Human Error","8.5","Very High","","","Limit switch adjusted to be operated.","2021-06-25T23:59:35","","Completed","2021-06-03T23:59:35","No","No","No","Internal"]
[null,null,null,19716,null,"50_16/06/2021 07:50:01","2021-05-27T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Port & stbd. lifeboat - 1 pc. of seat belt each found disconnected due to broken securing bolt.","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.29","High","","","Broken bolt removed & replaced with new one. Seat belts secured.","2021-06-10T23:59:35","","Completed","2021-05-27T23:59:35","No","No","No","Internal"]
[null,null,null,19717,null,"50_16/06/2021 17:22:52","2021-05-27T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Port provision crane block - Top plate found wasted.","Deck - Machinery","Cargo / Ballast Systems","External Factors","8.5","Very High","","","Top plate renewed & boxed back","2021-06-25T23:59:35","","Completed","2021-05-29T23:59:35","No","No","No","Internal"]
[null,null,null,19710,null,"50_16/06/2021 07:42:42","2021-05-27T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Fwd. liferaft & stbd. liferaft - several steps of embarkation ladder & rope found damaged.","LSA / FFA","Safety / LSA / FFA","External Factors","5.29","High","","","Requisition raised for new ladders.\n\nNew ladders received at Singapore on 8th July 2021.","2021-07-10T23:59:35","DPEO210133","Completed","2021-07-03T23:59:35","No","No","No","Internal"]
[null,null,null,19718,null,"50_16/06/2021 17:34:51","2021-05-28T23:59:35","Defect","Ship Staff","Ship Staff Insp.","No. 2 manifold stbd. side - Flange between manifold valve & inboard pipeline found leaking.","Deck - Pipe / Fittings","Cargo / Ballast Systems","External Factors","8.41","Medium","","","Entire section renewed. Flange body found corroded. Same cleaned up, derusted & painted. Gaskets renewed & entire section boxed back.","2021-06-10T23:59:35","","Completed","2021-06-06T23:59:35","No","No","No","Internal"]
[null,null,null,19723,null,"50_16/06/2021 17:30:44","2021-05-28T23:59:35","Observation","Ship Staff","Ship Staff Insp.","No. 2 manifold pressure gauge (Port side) showing steady pressure reading of 0 bar during discharging operation.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.41","Medium","","","Pressure gauge line from manifold side found chocked. Same cleared up.","2021-06-10T23:59:35","","Completed","2021-06-02T23:59:35","No","No","No","Internal"]
[null,null,null,19929,null,"50_02/07/2021 12:03:27","2021-05-28T23:59:35","Defect","Ship Staff","Ship Staff Insp.","2P & 2S aft COW machines found leaking on deck during COW operation.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.34","High","","","Both machine turbine shaft removed. Oil seal found damaged. Both seals renewed & turbine shaft boxed back.","2021-06-25T23:59:35","","Completed","2021-06-19T23:59:35","No","No","No","Internal"]
[null,null,null,19930,null,"50_02/07/2021 12:40:03","2021-05-28T23:59:35","Observation","Ship Staff","Ship Staff Insp.","3C aft COW machine found not operating during COW operations.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.34","High","","","Entire machine remove from the tank. Found nozzle clogged eith rust flakes & sludge. Nozzle cleared up & COW machine boxed back.","2021-06-25T23:59:35","","Completed","2021-06-23T23:59:35","No","No","No","Internal"]
[null,null,null,19719,null,"50_16/06/2021 19:31:56","2021-05-29T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Tank cleaning line supply valve - CAV154 found passing during discharging operation.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.44","High","","","Valve seat ring renewed in pump room.","2021-06-10T23:59:35","","Completed","2021-06-10T23:59:35","No","No","No","Internal"]
[null,null,null,19931,null,"50_02/07/2021 11:51:31","2021-05-29T23:59:35","Observation","Ship Staff","Ship Staff Insp.","No.1 and 2 cargo eductor suction gauge and no.1 cargo eductor disch. found stuck.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","Blockage cleared and pressure gauges calibrated of no.1 and 2 cargo eductor suction gauge and no.1 cargo eductor disch. Gauge.","2021-06-25T23:59:35","","Completed","2021-06-17T23:59:35","No","No","No","Internal"]
[null,null,null,19711,null,"50_16/06/2021 07:54:37","2021-05-31T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Port pilot ladder - Bottom rubber step found sagged & cracked. Last spreader step found twisted. Rope found damaged near the cracked rubber step.","Miscellaneous","Safety / LSA / FFA","External Factors","5.47","Medium","","","Requisition raised for new pilot ladder.\n\nNew ladder received at Singapore on 8th July 2021.","2021-07-10T23:59:35","DPEO210132","Completed","2021-06-03T23:59:35","No","No","No","Internal"]
[null,null,null,19720,null,"50_16/06/2021 17:40:40","2021-06-01T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Both port and starboard side lifeboat engine cooling pipe were found painted over thus reducing effectiveness of cooling.","LSA / FFA","Safety / LSA / FFA","Human Error","5.29","High","","","The paint over the cooling line was removed.","2021-06-25T23:59:35","","Completed","2021-06-09T23:59:35","No","No","No","Internal"]
[null,null,null,19712,null,"50_16/06/2021 19:37:28","2021-06-04T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Both HHC - Winch limit switches found inoperational.","Deck - Machinery","Cargo / Ballast Systems","External Factors","8.5","Very High","","","STBD HHC- WINCH LIMIT SWITCH MADE OPERATIONAL. \nPORT HHC- NEW CAM LIMIT SWITCH ASSEMBLY FITTED. NOW WINCH LIMIT SWITCH WORKING SATISFACTORY, \n","2023-02-10T23:59:35","DPEO220191","Completed","2023-04-23T23:59:35","No","No","No","Internal"]
[null,null,null,19713,null,"50_16/06/2021 20:01:25","2021-06-04T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Both HHC - Jerking observed during hoisting the winch while the operating lever is brought to stop.","Deck - Machinery","Cargo / Ballast Systems","Equipment Related","8.5","Very High","","","Presently working satisfactory, after putting the Limit switch hydraulic circuit in use.","2021-08-26T23:59:35","","Completed","2021-07-26T23:59:35","No","No","No","Internal"]
[null,null,null,19721,null,"50_16/06/2021 17:37:20","2021-06-04T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Seat ring of No. 2 manifold drain valve - stbd. side found damaged.","Deck - Pipe / Fittings","Cargo / Ballast Systems","External Factors","8.41","Medium","","","Seat ring renewed.","2021-06-10T23:59:35","","Completed","2021-06-05T23:59:35","No","No","No","Internal"]
[null,null,null,19724,null,"50_16/06/2021 19:21:40","2021-06-05T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Several thermometers of cargo manifolds were observed with damaged glasses & erroneous reading of temperature.","Miscellaneous","Cargo / Ballast Systems","External Factors","8.41","Medium","","","All thermometers renewed.","2021-06-25T23:59:35","","Completed","2021-06-09T23:59:35","No","No","No","Internal"]
[null,null,null,19722,null,"50_16/06/2021 19:27:37","2021-06-08T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Port HHC - Control lever block for slewing found leaking.","Deck - Mooring Machinery","Cargo / Ballast Systems","Equipment Related","8.5","Very High","","","Block removed for inspection. Condition og O-ring checked. Block boxed back & tightened up. Crane tried out & leak rectified.","2021-06-25T23:59:35","","Completed","2021-06-09T23:59:35","No","No","No","Internal"]
[null,null,null,19932,null,"50_02/07/2021 12:52:24","2021-06-11T23:59:35","Defect","Ship Staff","Ship Staff Insp.","No. 6 hydraulic box covers found wasted at several places.","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","External Factors","11.5","Medium","","","Covers removed & repairs carried out.","2021-06-23T23:59:35","","Completed","2021-06-23T23:59:35","No","No","No","Internal"]
[null,null,null,19922,null,"50_02/07/2021 13:05:43","2021-06-12T23:59:35","Observation","Ship Staff","Ship Staff Insp.","No. 1 foam monitor valve found leaking.","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.4","High","","","Gate valve dismantled,overhauled. working satisfactory.","2021-11-10T23:59:35","","Completed","2021-10-30T23:59:35","No","No","No","Internal"]
[null,null,null,19933,null,"50_02/07/2021 11:57:44","2021-06-16T23:59:35","Defect","Ship Staff","Ship Staff Insp.","WBT 2S (Aft) -  gas sampling flow fault.","Miscellaneous","Safety / LSA / FFA","Equipment Related","5.21","Medium","","","Sample line filters & flame arrestors found dirty with rust flakes. Both cleaned. Line blown through from CCR to deck & from deck to tank. System boxed back & tried out.","2021-06-25T23:59:35","","Completed","2021-06-17T23:59:35","No","No","No","Internal"]
[null,null,null,19934,null,"50_02/07/2021 12:44:40","2021-06-19T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Port lifeboat sprinkler valve could not be operated.","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.29","High","","","Upon inspection, it was observed that conecting rod to the sprinkler valve handle was disconnected. Same connected back.","2021-06-25T23:59:35","","Completed","2021-06-24T23:59:35","No","No","No","Internal"]
[null,null,null,19923,null,"50_01/07/2021 1:31:16 PM","2021-06-21T23:59:35","Defect","Ship Staff","Engineering Audit","The oil discharge valve of the OWS does not function satisfactory.","E/R - Aux. Mach.","MARPOL Related","Equipment Related","10.32","Very High","","","Spare valve recieved and tried out and found valve operation in order","2022-09-25T23:59:35","DPEO210115","Completed","2022-09-07T23:59:35","No","No","No","Internal","Spares are ready and will be supplied in Singapore."]
[null,null,null,19924,null,"50_01/07/2021 1:33:37 PM","2021-06-21T23:59:35","Defect","Ship Staff","Engineering Audit","The stop switch of boiler feed pump is defective","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","renewed with different stop switch working satisfactory","2021-09-21T23:59:35","DPEO210134","Completed","2021-07-30T23:59:35","No","No","No","Internal"]
[null,null,null,19925,null,"50_01/07/2021 1:36:36 PM","2021-06-21T23:59:35","Defect","Ship Staff","Engineering Audit","Purifier filter cartridge bridge found cracked and temporarily welded","Deck - Pipe / Fittings,E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Renewed filter cartridge bridge from spare.","2021-12-20T23:59:35","DPEO210091","Completed","2022-01-03T23:59:35","No","No","No","Internal"]
[null,null,null,19926,null,"50_01/07/2021 1:39:46 PM","2021-06-21T23:59:35","Defect","Ship Staff","Engineering Audit","Flourescent light circuit to convert to LED Light.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Knowledge Based","10.37","Medium","","","Lights and circuit converted.","2021-11-23T23:59:35","DPEO210113","Completed","2021-11-30T23:59:35","No","No","No","Internal"]
[null,null,null,19927,null,"50_01/07/2021 1:43:26 PM","2021-06-21T23:59:35","Defect","Ship Staff","Engineering Audit","Compressor found to trip on high temperature & Oil discharge hose renewed with fabricated one.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","renewed hose and filter tried out satisfactory","2021-09-20T23:59:35","DPEO210097","Completed","2021-07-30T23:59:35","No","No","No","Internal"]
[null,null,null,19928,null,"50_02/07/2021 13:02:14","2021-06-21T23:59:35","Defect","Ship Staff","Ship Staff Insp.","2 fireman's helmets found with damaged head bands. One of these helmet hard hat found cracked. ","LSA / FFA","Safety / LSA / FFA","External Factors","5.43","High","","","New helmet & head band received.","2021-07-25T23:59:35","DPEO210148","Completed","2021-07-24T23:59:35","No","No","No","Internal"]
[null,null,null,19935,null,"50_02/07/2021 12:47:32","2021-06-23T23:59:35","Observation","Ship Staff","Ship Staff Insp.","WBT 1S (fwd.) -  gas sampling flow fault.","Miscellaneous","Safety / LSA / FFA","Equipment Related","5.21","Medium","","","Sample line filters & flame arrestors found dirty with rust flakes. Both cleaned. Line blown through from CCR to deck & from deck to tank. System boxed back & tried out.","2021-06-25T23:59:35","","Completed","2021-06-25T23:59:35","No","No","No","Internal"]
[null,null,null,20314,null,"50_23/07/2021 09:37:49","2021-06-30T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Rain water from external C deck port side found leaking into E/boy's cabin toilet.","Accommodation","Structural Condn. / WT integrity ","External Factors","11.13","Low","","","Soft repair carried out on 2 wasted sections of drain on external C deck ","2021-07-10T23:59:35","","Completed","2021-07-06T23:59:35","No","No","No","Internal"]
[null,null,null,20315,null,"50_23/07/2021 08:08:40","2021-07-02T23:59:35","Observation","Ship Staff","Ship Staff Insp.","C deck spare cabin wash basin drain pipe found leaking.\t","Miscellaneous","Structural Condn. / WT integrity ","Equipment Related","","","","","Drain pipe renewed.","2021-07-10T23:59:35","","Completed","2021-07-10T23:59:35","No","No","No","Internal"]
[null,null,null,20310,null,"50_02/08/2021 21:35:21","2021-07-03T23:59:35","Defect","Ship Staff","Ship Staff Insp.","4S WBT stripper valve flange was observed to be seeping as rubber gasket was damaged","Miscellaneous","Cargo / Ballast Systems","External Factors","8.11","Medium","","","Rubber gasket renewed. ","2021-12-25T23:59:35","DPEO210160","Completed","2021-12-04T23:59:35","No","No","No","Internal"]
[null,null,null,20311,null,"50_02/08/2021 22:09:27","2021-07-07T23:59:35","Defect","Ship Staff","Ship Staff Insp.","IG to cargo valve was found not holding during pressure testing","Deck - Pipe / Fittings","Cargo / Ballast Systems","External Factors","8.41","Medium","","","Nuts and bolts renewed. ","2021-09-25T23:59:35","DPEO210088","Completed","2021-09-23T23:59:35","No","No","No","Internal"]
[null,null,null,20312,null,"50_02/08/2021 22:12:44","2021-07-07T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Slop P COW line drain valve observed to be passing.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.34","High","","","Leaking gate valve replaced with new gate valve received at singapore.","2021-09-25T23:59:35","DPEO210088 ","Completed","2021-09-25T23:59:35","No","No","No","Internal"]
[null,null,null,20316,null,"50_23/07/2021 07:19:58","2021-07-07T23:59:35","Defect","Ship Staff","Ship Staff Insp.","2P no.3 COW machine branch valve found leaking from spindle during pressure testing.\t","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.34","High","","","Gland packing renewed.","2021-07-10T23:59:35","","Completed","2021-07-08T23:59:35","No","No","No","Internal"]
[null,null,null,20317,null,"50_23/07/2021 07:22:56","2021-07-07T23:59:35","Defect","Ship Staff","Ship Staff Insp.","2S no.3 COW machine found leaking from turbine gear box.\t","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.34","High","","","On further inspection, spring washer found damaged. New spring washer installed.","2021-07-10T23:59:35","","Completed","2021-07-08T23:59:35","No","No","No","Internal"]
[null,null,null,20318,null,"50_23/07/2021 08:51:42","2021-07-07T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Port side manifold drip tray drain plug found loose cause of bad condition of threads of drip tray drain. Also drain found blocked with silicon.","Deck - Pipe / Fittings","Cargo / Ballast Systems","External Factors","","","","","Drip tray and drain plug both drain plug tapped. Arrangement modified by installing small valve. Same arrangement made on stbd. side drip tray. ","2021-07-10T23:59:35","","Completed","2021-07-09T23:59:35","No","No","No","Internal"]
[null,null,null,20319,null,"50_02/08/2021 21:38:23","2021-07-07T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Leak observed from stripper pump steam glands","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.8","Medium","","","Gland packing renewed & leak rectified.","2021-07-12T23:59:35","","Completed","2021-07-09T23:59:35","No","No","No","Internal"]
[null,null,null,20320,null,"50_02/08/2021 21:55:02","2021-07-08T23:59:35","Observation","Ship Staff","Ship Staff Insp.","WBT 1S (F) 2S(A), 4S(A), 5S(A) and void space of pumproom (S) -  gas sampling flow fault.","Miscellaneous","Safety / LSA / FFA","Equipment Related","5.21","Medium","","","Sample line filters & flame arrestors found dirty with rust flakes. Both cleaned. Line blown through from CCR to deck & from deck to tank. System boxed back & tried out.","2021-07-25T23:59:35","","Completed","2021-07-10T23:59:35","No","No","No","Internal"]
[null,null,null,20313,null,"50_03/08/2021 5:14:45 PM","2021-07-13T23:59:35","Defect","Ship Staff","Engineering Audit","Aft bellow for turbocharger is cracked needs replacement","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Flanges new holes drilled and renewed the aft bellow.","2022-01-13T23:59:35","DPEO215111","Completed","2021-11-01T23:59:35","No","No","No","Internal"]
[null,null,null,20321,null,"50_02/08/2021 22:01:15","2021-07-14T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Various COW machine branch valves found leaking from spindle during COW operation.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.34","High","","","Gland packing renewed.","2021-07-25T23:59:35","","Completed","2021-07-18T23:59:35","No","No","No","Internal"]
[null,null,null,20790,null,"50_03/09/2021 12:35:54 PM","2021-07-24T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","EGE Exhaust gas leaking from the base.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Leakage arrested.","2021-12-24T23:59:35","","Completed","2021-11-06T23:59:35","No","No","No","Internal"]
[null,null,null,20392,null,"50_14/08/2021 14:04:11","2021-07-24T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Hydraulic pipes clamps and support in rusted condition.","Deck - Pipe / Fittings","General Appearance","Equipment Related,External Factors","","","","","Derusting, buffing and painting is in progress.","2021-10-26T23:59:35","","Completed","2021-10-19T23:59:35","No","No","No","Internal"]
[null,null,null,20393,null,"50_14/08/2021 14:36:05","2021-07-24T23:59:35","Critical Equipment,Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Fire lines on deck & flanges rusted","LSA / FFA","Emgcy. Systems","Equipment Related,External Factors","","","","","Derusting, buffing and painting completed.","2021-11-25T23:59:35","","Completed","2021-11-25T23:59:35","No","No","No","Internal"]
[null,null,null,20394,null,"50_14/08/2021 14:40:47","2021-07-24T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Main deck rusted at scattered location,peeling off paint due to bad surface preparation.","Deck - Pipe / Fittings","General Appearance","External Factors","","","","","Derusting, buffing completed. Full coat of main deck painting is in progress.","2021-12-25T23:59:35","","Completed","2021-12-18T23:59:35","No","No","No","Internal"]
[null,null,null,20395,null,"50_14/08/2021 14:45:19","2021-07-24T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","All PV valves flanges rusted.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related,External Factors","","","","","Derusting, buffing and painting carried out","2021-09-24T23:59:35","","Completed","2021-09-24T23:59:35","No","No","No","Internal"]
[null,null,null,20396,null,"50_14/08/2021 14:50:46","2021-07-24T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Midship mast sidelights frame and brackets rusted.","Navigation - Others","Navigation","Equipment Related,External Factors","","","","","Derusting, buffing and painting  carried out.","2021-09-03T23:59:35","","Completed","2021-08-20T23:59:35","No","No","No","Internal"]
[null,null,null,20397,null,"50_14/08/2021 19:23:32","2021-07-24T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Fire hose box on deck have loose doors ","LSA / FFA","Emgcy. Systems","Equipment Related,Human Error","","","","","All fire hose boxes door tightened.","2021-09-24T23:59:35","","Completed","2021-08-17T23:59:35","No","No","No","Internal"]
[null,null,null,20398,null,"50_14/08/2021 19:28:56","2021-07-24T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","crutches for luffing boom rest on top of midship store rusted","Deck - Machinery","General Appearance","Equipment Related,Human Error,Inappropriate Procedure","","","","","derusting and painting completed.","2021-11-25T23:59:35","","Completed","2021-11-25T23:59:35","No","No","No","Internal"]
[null,null,null,20399,null,"50_15/08/2021 21:51:26","2021-07-24T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","IG Mast riser pipes and flanges rusted","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related,External Factors","8.4","Medium","","","Derusting & painting completed","2022-09-10T23:59:35","","Completed","2022-08-26T23:59:35","No","No","No","Internal"]
[null,null,null,20400,null,"50_15/08/2021 21:56:59","2021-07-24T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Gasket channel rusted of  hydraulic boxes 3A/B & 2A/B on deck","Cargo Mach.","Cargo / Ballast Systems","Equipment Related,External Factors","","","","","spot derusting and painting carried out","2021-09-25T23:59:35","","Completed","2021-09-20T23:59:35","No","No","No","Internal"]
[null,null,null,20401,null,"50_15/08/2021 22:05:48","2021-07-24T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","In windlass brake cylinder indicator position not matching with spindle position","Deck - Mooring Machinery","Mooring","Equipment Related,External Factors","","","","","All break indicator adjusted.","2021-08-24T23:59:35","","Completed","2021-08-12T23:59:35","No","No","No","Internal"]
[null,null,null,20402,null,"50_15/08/2021 22:25:25","2021-07-24T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Windlass / Mooring winches brake band stopper bolt clearence varying from 03mm to 10mm on various winches. paint to be removed from bolts","Deck - Mooring Machinery","Mooring","Equipment Related,External Factors","","","","","All break band stopper adjusted. Paint removed from bolts.","2021-08-13T23:59:35","","Completed","2021-08-12T23:59:35","No","No","No","Internal"]
[null,null,null,20403,null,"50_16/08/2021 14:32:48","2021-07-24T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Main deck walkway supports fwd of manifold are rusted.","Deck - Pipe / Fittings","General Appearance","External Factors","","","","","Spot derusting and painting is completed.","2021-09-25T23:59:35","","Completed","2021-09-25T23:59:35","No","No","No","Internal"]
[null,null,null,20404,null,"50_16/08/2021 14:39:23","2021-07-24T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","On main deck walkway support cable having pvc/plastic cover were rusted fro inside.","Deck - Pipe / Fittings","General Appearance","Equipment Related,External Factors","","","","","Rusted walkway support cables  replaced.","2021-09-25T23:59:35","","Completed","2021-09-25T23:59:35","No","No","No","Internal"]
[null,null,null,20405,null,"50_16/08/2021 14:46:48","2021-07-24T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Butterworth & COT manhole covers are rusted.","Deck - Pipe / Fittings","General Appearance","External Factors","","","","","Spot derusting and  complete painting carried out.","2021-10-26T23:59:35","","Completed","2021-10-26T23:59:35","No","No","No","Internal"]
[null,null,null,20406,null,"50_16/08/2021 14:50:13","2021-07-24T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Slop tank heating coil steam manifold valve is rusted","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related,External Factors","","","","","Spot derusting and painting  carried out.","2021-09-25T23:59:35","","Completed","2021-09-23T23:59:35","No","No","No","Internal"]
[null,null,null,20407,null,"50_16/08/2021 14:58:48","2021-07-24T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Steam pipe on main deck near slop port COT rusted.","Deck - Pipe / Fittings","General Appearance","External Factors","","","","","Spot derusting and Painting  carried out.","2021-09-25T23:59:35","","Completed","2021-09-23T23:59:35","No","No","No","Internal"]
[null,null,null,20408,null,"50_16/08/2021 15:02:54","2021-07-24T23:59:35","Critical Equipment,Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","All  Foam monitor's flanges and valves rusted.","LSA / FFA","Safety / LSA / FFA","Equipment Related,External Factors","","","","","Spot derusting and Painting carried out.","2021-09-25T23:59:35","","Completed","2021-09-25T23:59:35","No","No","No","Internal"]
[null,null,null,20409,null,"50_16/08/2021 15:08:35","2021-07-24T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Fire hose box installed near EGB soot blower is fully dirty.","LSA / FFA","General Appearance","Behaviour Based,External Factors","","","","","Fire hose box  cleaned","2021-08-10T23:59:35","","Completed","2021-08-09T23:59:35","No","No","No","Internal"]
[null,null,null,22498,null,"50_23/10/2021 10:40:13 PM","2021-07-24T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Chemical dosing pump for Auxiliary boiler area looks dirty.","E/R - Pipes/ valves & fittings","General Appearance","Equipment Related","10.29","Medium","","","Cleaned and painted the area","2021-08-05T23:59:35","","Completed","2021-08-04T23:59:35","No","No","No","Internal"]
[null,null,null,22499,null,"50_23/10/2021 10:42:32 PM","2021-07-24T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Aft hyd. system filter clogging alarm active","Deck - Mooring Machinery","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Renewed the filter and tried out found satisfactory","2021-08-10T23:59:35","","Completed","2021-08-09T23:59:35","No","No","No","Internal"]
[null,null,null,22500,null,"50_23/10/2021 10:44:58 PM","2021-07-24T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Ship Staff Insp.","Fire hose box near soot blower dirty","Miscellaneous","General Appearance","External Factors","10.29","Medium","","","Cleaned the Box","2021-08-10T23:59:35","","Completed","2021-08-07T23:59:35","No","No","No","Internal"]
[null,null,null,22501,null,"50_23/10/2021 10:46:50 PM","2021-07-24T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","AE 3 FCU unit exterior looks dirty","E/R - Pipes/ valves & fittings","General Appearance","External Factors","10.29","Medium","","","Checked for leaks found non, Old oil stains noticed, same cleaned and painted.","2021-08-10T23:59:35","","Completed","2021-08-07T23:59:35","No","No","No","Internal"]
[null,null,null,22502,null,"50_23/10/2021 10:49:11 PM","2021-07-24T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Emergency generator exhaust pipe external holed.","E/R - Pipes/ valves & fittings","General Appearance","External Factors","10.32","Very High","","","Renewed the corroded pipe","2021-08-15T23:59:35","","Completed","2021-08-14T23:59:35","No","No","No","Internal"]
[null,null,null,20998,null,"50_14/09/2021 4:38:48 PM","2021-08-28T23:59:35","Defect","Ship Staff","Engineering Audit","Auxiliary boiler Feed water pump ammeter not in operation","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Renewed on receiving the spare","2022-01-12T23:59:35","DPEO210136","Completed","2022-01-06T23:59:35","No","No","No","Internal"]
[null,null,null,22503,null,"50_03/11/2021 5:36:22 AM","2021-09-04T23:59:35","Observation","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","The E/R Log book was not adequately maintained. Various errors were made in the book for the month of August 2021 either by overwritten or stuck through with a single line but without initialled and date.","Miscellaneous","ISM Related","External Factors","10.5","Low","","","All Engine staff briefed on importance of filling the E/R log book in a proper manner as it is official. Training for the same carried out.","2021-12-03T23:59:35","","Completed","2021-09-05T23:59:35","No","No","No","External"]
[null,null,null,21377,null,"50_02/10/2021 15:32:05","2021-09-12T23:59:35","Breakdown,Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Few Inert gas supply valve to cargo tanks found leaking and gear mechanism broken.","Cargo Mach.,Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.3","Very High","","","Maintance and Inspection is in progress. 6 seat rings renewed and RO raised for new valves and seat rings, awaiting Supply\n\nNew DDRL job created consolidating all IG branch valves issues","2023-05-26T23:59:35","DPEO220050","Completed","2022-02-16T23:59:35","No","No","No","Internal"]
[null,null,null,21378,null,"50_02/10/2021 15:36:15","2021-09-12T23:59:35","Breakdown,Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Level gauge of 1S WBT,5S WBT & APT tanks found giving erratic reading.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","Presently working satisfactory","2022-01-25T23:59:35","","Completed","2022-01-01T23:59:35","No","No","No","Internal"]
[null,null,null,21380,null,"50_02/10/2021 15:41:13","2021-09-12T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Mast light fittings on main deck of incorrect fittings and light can not be directed correctly on deck.","Deck - Pipe / Fittings","Safety / LSA / FFA","Equipment Related","","","","","Installation carried out.","2021-11-25T23:59:35","","Completed","2021-10-20T23:59:35","No","No","No","Internal"]
[null,null,null,22489,null,"50_23/10/2021 9:58:35 PM","2021-09-12T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Areas on top of air trunkings/pipelines/Ship sides needs to be cosmetically upgraded","Miscellaneous","General Appearance","External Factors","10.29","Medium","","","Cleaned and painted as required.","2021-11-25T23:59:35","","Completed","2021-11-25T23:59:35","No","No","No","Internal"]
[null,null,null,22490,null,"50_23/10/2021 10:30:22 PM","2021-09-12T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Steam header lines insulation found damaged and not fully covered","Miscellaneous","General Appearance","External Factors","10.19","Very High","","","Insulation material ordered awaiting supply of insulation material for covering.","2022-02-23T23:59:35","DPEO210208","Completed","2022-01-07T23:59:35","No","No","No","Internal","Please order Insulation material under stores."]
[null,null,null,22504,null,"50_22/10/2021 9:28:21 PM","2021-09-12T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Hyper mist light source found to be dim","LSA / FFA","Safety / LSA / FFA","Equipment Related","8.69","Medium","","","The original bulb was LED same was replaced with ordinary bulb arrangement for brighter indication.","2021-12-14T23:59:35","","Completed","2021-09-22T23:59:35","No","No","No","Internal"]
[null,null,null,22505,null,"50_22/10/2021 9:32:51 PM","2021-09-12T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Heat detector above Auxiliary boiler was given external duct ","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.31","High","","","The duct was placed as due to hot air of engine room false alarm was being triggered, The duct is removed.","2021-09-22T23:59:35","","Completed","2021-09-15T23:59:35","No","No","No","Internal"]
[null,null,null,22506,null,"50_22/10/2021 9:41:36 PM","2021-09-12T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","AC unit condenser pipes looks dirty","Miscellaneous","Eng. / Strg. Comp.","External Factors","10.29","Medium","","","Cleaned and  painted the pipeline","2021-09-24T23:59:35","","Completed","2021-09-23T23:59:35","No","No","No","Internal"]
[null,null,null,22507,null,"50_23/10/2021 2:40:05 AM","2021-09-12T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Welding cable not coiled and secured properly","Miscellaneous","ISM Related","Human Error","5.25","Medium","","","Welding cable coiled and stored properly","2021-09-24T23:59:35","","Completed","2021-09-18T23:59:35","No","No","No","Internal"]
[null,null,null,22508,null,"50_23/10/2021 9:22:16 PM","2021-09-12T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","AHU Housing looks dirty","Miscellaneous","General Appearance","External Factors","10.29","Medium","","","Washed and repainted.","2021-10-27T23:59:35","","Completed","2021-09-18T23:59:35","No","No","No","Internal"]
[null,null,null,22509,null,"50_23/10/2021 9:26:33 PM","2021-09-12T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","No.2 HP Circulating pump is observed to be vibrating and disharge pressure gauge not visible","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Tightened the pump base to arrest the vibration and renewed the pressure gauge.","2021-10-27T23:59:35","","Completed","2021-09-25T23:59:35","No","No","No","Internal"]
[null,null,null,22510,null,"50_23/10/2021 9:32:23 PM","2021-09-12T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Pump room blower sensor wires found coiled shabbily in E/R","Elect. Mach. & Equip.","General Appearance","External Factors","11.1","High","","","Cable removed and coiled and secured properly.","2021-09-26T23:59:35","","Completed","2021-09-22T23:59:35","No","No","No","Internal"]
[null,null,null,22511,null,"50_23/10/2021 10:04:17 PM","2021-09-12T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","A/E No.2 Oil max pump was not running","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Pump renewed from spare","2021-09-26T23:59:35","","Completed","2021-09-15T23:59:35","No","No","No","Internal"]
[null,null,null,22512,null,"50_23/10/2021 10:06:59 PM","2021-09-12T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Auxiliary boiler gauge glass remote valve release wires seized","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Eased up the lines for remote operation and tried out found working satisfactory.","2021-09-26T23:59:35","","Completed","2021-09-22T23:59:35","No","No","No","Internal"]
[null,null,null,22513,null,"50_23/10/2021 10:32:30 PM","2021-09-12T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Feed water tank looks dirty","Miscellaneous","General Appearance","External Factors","10.29","Medium","","","Cleaned and painted the tank.","2021-10-11T23:59:35","","Completed","2021-09-20T23:59:35","No","No","No","Internal"]
[null,null,null,22514,null,"50_23/10/2021 10:34:26 PM","2021-09-12T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","EEBD in E/R looks dirty","Miscellaneous","General Appearance","External Factors","10.29","Medium","","","Cleaned and stowed safely.","2021-09-23T23:59:35","","Completed","2021-09-22T23:59:35","No","No","No","Internal"]
[null,null,null,21379,null,"50_02/10/2021 8:58:18 PM","2021-09-14T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Steam injector valve bonnet leaking near fresh water generator","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Renewed the gasket","2021-12-25T23:59:35","","Completed","2021-10-02T23:59:35","No","No","No","Internal"]
[null,null,null,22491,null,"50_03/11/2021 5:50:49 AM","2021-10-13T23:59:35","Observation","Ship Staff","Engineering Audit","Incinerator exhaust controller and air suction controller flaps not working.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","The controller found not working, needs replacement.  Spar recieved and replaced .","2022-12-26T23:59:35","DPEO220038","Completed","2022-06-25T23:59:35","No","No","No","Internal","Noted, will process requisition."]
[null,null,null,22492,null,"50_03/11/2021 6:54:12 AM","2021-10-13T23:59:35","Observation","Ship Staff","Engineering Audit","Gas leaking from EGB Byepass valve bearing. The bearing and seal needs renewal.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Seal arrangment tightened and no leaks observed","2022-09-25T23:59:35","DPEO220081","Completed","2022-08-27T23:59:35","No","No","No","Internal","Noted."]
[null,null,null,22493,null,"50_03/11/2021 6:57:10 AM","2021-10-13T23:59:35","Defect","Ship Staff","Ship Staff Insp.","M/E and A/E Fuel viscosity sensors failure","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","M/E and A/E Fuel viscosity sensor was cleaned and checked all the connections including the fuses. After resuming connection system started to give proper readings.","2023-10-03T23:59:35","DPEO230230 - Cancelled","Completed","2023-10-10T23:59:35","No","No","No","Internal","Please trouble shoot and share full details. One liner will not help us to understand."]
[null,null,null,22494,null,"50_03/11/2021 6:59:26 AM","2021-10-13T23:59:35","Observation","Ship Staff","Ship Staff Insp.","M/E Load indicator showing fluctuation in indication","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","LOAD INDICATOR  LINKAGES CONNECTING FASTENERS TIGTENED(FOUND LOOSE), NOW  NO FLUCTUATION","2022-12-25T23:59:35","DPEO220266 - ME LOAD INDICATOR TRANSMITTER","Completed","2023-01-06T23:59:35","No","No","No","Internal","ordered. awaiting readiness."]
[null,null,null,22495,null,"50_03/11/2021 7:03:04 AM","2021-10-13T23:59:35","Defect","Ship Staff","Ship Staff Insp.","M/E Cylinder lubricating pump found to pulse start continuously.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Renewed from spare","2022-01-12T23:59:35","DPEO210213","Completed","2021-11-06T23:59:35","No","No","No","Internal"]
[null,null,null,22496,null,"50_03/11/2021 7:05:23 AM","2021-10-13T23:59:35","Observation","Ship Staff","Ship Staff Insp.","No.2 IG Oxygen sensor system filter missing","Inert Gas","Eng. / Strg. Comp.","External Factors","10.32","Very High","","","Filter found and renewed.","2022-01-12T23:59:35","DPEO210210","Completed","2021-11-21T23:59:35","No","No","No","Internal"]
[null,null,null,22497,null,"50_03/11/2021 7:11:36 AM","2021-10-13T23:59:35","Observation","Ship Staff","Ship Staff Insp.","No.2 Main Air compressor HP piston mildly damaged, needs replacement","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Received spares. Boxed back after inspection and calibration. Tried out. Working satisfactory.","2022-02-23T23:59:35","","Completed","2022-02-22T23:59:35","No","No","No","Internal","Noted."]
[null,null,null,23239,null,"50_17/12/2021 12:43:44 AM","2021-11-26T23:59:35","Defect","Ship Staff","Engineering Audit","M/E Unit no.1 Port side blank quills found leaking off water","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Renewed the O-rings and arrested the leaks","2022-02-24T23:59:35","","Completed","2022-01-11T23:59:35","No","No","No","Internal"]
[null,null,null,23240,null,"50_17/12/2021 12:42:16 AM","2021-11-26T23:59:35","Defect","Ship Staff","Engineering Audit","Buffer tank Gauge glass top portion leaking mildly off air","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Tightened mildly, but need to isolate the Jacket water system to renew the leaking gauge glass. To be carried out at convenient anchorage.","2022-02-24T23:59:35","","Completed","2022-01-19T23:59:35","No","No","No","Internal"]
[null,null,null,23241,null,"50_17/12/2021 12:47:25 AM","2021-11-26T23:59:35","Defect","Ship Staff","Engineering Audit","MDO storage tank, MDO Settling and service tanks remote gauges not working","Hull & Tanks","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Remote level gauge replaced with newly received lavel gauge. Level compared with actual sounding. Found to be correct. Remote level Gauge replaced with all three MDO Tanks.","2022-07-26T23:59:35","DPEO220018","Completed","2022-07-20T23:59:35","No","No","No","Internal"]
[null,null,null,23242,null,"50_17/12/2021 1:06:38 AM","2021-11-26T23:59:35","Defect","Ship Staff","Engineering Audit","FWG Condenser cover and bottom evaporator cover has got hole same to raise requisition and renew the same.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Replaced condensor bottom end cover and evaporator SW side both end covers. Tried out. No leaks.","2022-02-24T23:59:35","DPEO210102","Completed","2022-02-22T23:59:35","No","No","No","Internal","Supplied in Singapore."]
[null,null,null,23243,null,"50_31/12/2021 12:22:02 PM","2021-12-11T23:59:35","Defect","Ship Staff","Engineering Audit","Deck air compressor suction valve plate not in good condition, needs replacement","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Renewed and working satisfactory","2022-03-10T23:59:35","DPEO210222","Completed","2022-01-05T23:59:35","No","No","No","Internal","Spares supplied to vsl."]
[null,null,null,23244,null,"50_31/12/2021 12:44:21 PM","2021-12-11T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Pump room manual fire call point box external is cracked, needs replacement","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.32","High","","","Received new spare, the alarm gets activated but fire bell is not ringing in the accomodation. Correspondence with office in progress.","2022-03-10T23:59:35","DPEO210189","Completed","2022-01-27T23:59:35","No","No","No","Internal"]
[null,null,null,23245,null,"50_31/12/2021 12:46:59 PM","2021-12-11T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Cargo oil pump no.2 vibration sensor probe defective","Deck - Machinery","Eng. / Strg. Comp.","Equipment Related","8.18","High","","","Spare received and COPT no.2 vibration sensor renewed.","2022-05-26T23:59:35","DPEO220005","Completed","2022-05-21T23:59:35","No","No","No","Internal"]
[null,null,null,23247,null,"50_31/12/2021 12:27:07 PM","2021-12-11T23:59:35","Defect","Ship Staff","Engineering Audit","PAH Sensor for Sox water outlet is not working satisfactory","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Renewed with new found working satisfactory","2022-03-10T23:59:35","DPEO215127","Completed","2022-01-19T23:59:35","No","No","No","Internal"]
[null,null,null,23246,null,"50_31/12/2021 12:19:13 PM","2021-12-22T23:59:35","Defect","Ship Staff","Engineering Audit","Steering gear servo filter micro switch giving false alarm","Elect. Mach. & Equip.","Eng. / Strg. Comp.","External Factors","10.39","High","","","Renewed switch found working satisfactory.","2022-03-21T23:59:35","DPEO210246","Completed","2022-01-03T23:59:35","No","No","No","Internal","Spares supplied. Please carryout the repair and close the observation"]
[null,null,null,23724,null,"50_15/01/2022 3:52:26 PM","2022-01-02T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Flame detector tester not working satisfactory due to week battery","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.39","Very High","","","\n\nReceived spare and tested found working satisfactory.","2022-04-01T23:59:35","DPEO210236","Completed","2022-01-12T23:59:35","No","No","No","Internal","spares are ready and will be connected to vsl  at next port."]
[null,null,null,23731,null,"50_15/01/2022 3:55:41 PM","2022-01-02T23:59:35","Non Conformity","Ship Staff","Ship Staff Insp.","Test gas certificate for test gas of fixed oxygen analyser is expired.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","8.26","High","","","Replaced new N2 bottle with test certificate","2022-04-01T23:59:35","DPEO220086","Completed","2022-03-15T23:59:35","No","No","No","Internal"]
[null,null,null,23725,null,"50_13/01/2022 11:29:30","2022-01-07T23:59:35","Defect","Ship Staff","Ship Staff Insp.","All level sight glass of mooring winches gear oil tank looks hazy. Difficult to see oil level inside the gear oil tank.","Deck - Mooring Machinery","Mooring","Equipment Related","9.14","Medium","","","Cleaning of all level sight glass of mooring winches &  windlass gear oil completed.","2022-07-26T23:59:35","","Completed","2022-07-09T23:59:35","No","No","No","Internal","Please collect  oil and try to clean the gauge glass. Order only for those glasses which cannot be cleaned or reused."]
[null,null,null,23726,null,"50_13/01/2022 12:04:18","2022-01-07T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Both HHC have jerking issues occasionally.","Deck - Machinery","Cargo / Ballast Systems","Equipment Related","8.63","High","","","Spare received  & the spool of hoisting control lever block renewed on both HHC","2022-04-25T23:59:35","DPEO220003","Completed","2022-04-23T23:59:35","No","No","No","Internal","spares supplied on 07 Feb 2022."]
[null,null,null,23727,null,"50_13/01/2022 12:07:56","2022-01-07T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Mud sediments in all ballast tanks. Approximate quantity around 50 MT each tank","Hull & Tanks","Cargo / Ballast Systems","External Factors","2.9","Medium","","","All tanks to be cleaned.\n- Mud sediments in all Ballast tank are in acceptable limit  Hence job is shown as completed","2022-12-10T23:59:35","","Completed","2022-11-26T23:59:35","No","No","No","Internal"]
[null,null,null,23729,null,"50_15/01/2022 4:04:15 PM","2022-01-07T23:59:35","Observation","Ship Staff","Ship Staff Insp.","If the oxygen content is above 5%, still the Inert gas to deck would not be stopped. ","Inert Gas","Cargo / Ballast Systems","Equipment Related","8.26","High","","","The control system settings modified as per office advice and valve shuts down above 5% .","2022-11-25T23:59:35","","Completed","2022-11-07T23:59:35","No","No","No","Internal"]
[null,null,null,23730,null,"50_15/01/2022 16:46:37","2022-01-09T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Elevator malfunctioning","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","SEVICE TECHENICIAN ATTEND THE ELEVATOR. CONNECTION CABLE FOUND DEFECTIVE. SAME CONNECTED WITH SAPE CABLE. VARIOUS SPARE RENEWED BY THE SERVICE TECHANICIAN. OPERATON OF ELEVATOR CONFIRMED FROM ALL DECK. JOB HAS BEEN CARRIED OUT AT FUJAIRAH ON 05 MARCH 2022. \nAT PRESENT ELEVATOR OPERATION IS SATISFACTORY.","2022-07-26T23:59:35","DPEO225023, DPEO220136","Completed","2022-02-28T23:59:35","No","No","No","Internal","Office has raised PO and spares are ready. will be supplied in Singapore in 1st week of FEB."]
[null,null,null,23834,null,"50_25/01/2022 10:36:58 AM","2022-01-13T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Cargo pump mechanical seal alarm showing in CCR due to fault in Zener barrier unit","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.8","Medium","","","COPT NO. 2, VIBRATION DETECT MONITOR RECEIVED AND RENEWED.","2022-05-25T23:59:35","DPEO220005","Completed","2022-05-21T23:59:35","No","No","No","Internal"]
[null,null,null,23835,null,"50_30/01/2022 12:26:45 PM","2022-01-24T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Scrubber SW. Overboard valve leaking","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.31","Very High","","","Renewed the valve at singapore. ","2023-02-23T23:59:35","DPEO220051","Completed","2023-03-18T23:59:35","No","No","No","Internal","ting correct valve size from makers."]
[null,null,null,24511,null,"50_22/3/2022 10:41:45 AM","2022-02-16T23:59:35","Observation","Ship Staff","Suptd. Insp.","Rusted U clamps on deck pipelines","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.4","Very High","","","NEED TO DE-RUST ALL U CLAMPS ON PIPE LINES AND REPLACE AS NEEDED. CHECK INVENTORY AND RAISE PO AS REQ’D. \nSHIP’S STAFF COMMENT: NEW U-CLAMPS RECEIVED. DERUSTING IN COMPLETED\n","2023-01-10T23:59:35","","Completed","2023-02-10T23:59:35","No","No","No","Internal"]
[null,null,null,24512,null,"50_22/03/2022 15:11:37","2022-02-16T23:59:35","Observation","Ship Staff","Suptd. Insp.","Steam pipe for mast riser pipe corroded.","Deck - Machinery","General Appearance","Equipment Related","11.4","Very High","","","De-rusting and painting of steam pipe carried out.  Wasted lengths renewed with new fabricated lengths.","2022-11-10T23:59:35","","Completed","2022-10-25T23:59:35","No","No","No","Internal"]
[null,null,null,24513,null,"50_22/03/2022 15:22:56","2022-02-16T23:59:35","Observation","Ship Staff","Suptd. Insp.","Mooring winch hyd. pipe line flanges on HP are corroded.","Deck - Mooring Machinery","Mooring","Equipment Related","11.4","Very High","","","DERUSTING & PAINTING OF MOORING WINCH HYD. PIPE LINE FLANGES ON HP CARRIED OUT.","2022-10-10T23:59:35","","Completed","2022-10-03T23:59:35","No","No","No","Internal"]
[null,null,null,24515,null,"50_22/03/2022 15:46:51","2022-02-16T23:59:35","Observation","Ship Staff","Suptd. Insp.","Check Mast riser breather valve for operation","Inert Gas","Cargo / Ballast Systems","Equipment Related","8.19","High","","","MAST RISER BREATHER VALVE INSPECTION CARRIED OUT, CLEANED AND NO BLANK FOUND.","2022-04-25T23:59:35","","Completed","2022-04-04T23:59:35","No","No","No","Internal"]
[null,null,null,24516,null,"50_22/03/2022 16:31:29","2022-02-16T23:59:35","Observation","Ship Staff","Suptd. Insp.","STBD windlass, inspect bearing and renew if damaged.","Deck - Mooring Machinery","Mooring","Equipment Related","9.2","Very High","","","Stbd Windlass Bearings renewed and greased. Working satisfactory. ","2022-06-25T23:59:35","","Completed","2022-03-13T23:59:35","No","No","No","Internal"]
[null,null,null,24517,null,"50_22/03/2022 16:52:46","2022-02-16T23:59:35","Observation","Ship Staff","Suptd. Insp.","Mooring winches operating block to be de rusted","Deck - Mooring Machinery","Mooring","Equipment Related","9.14","Medium","","","De-rusting & painting of Mooring winch blocks completed","2022-10-10T23:59:35","","Completed","2022-10-03T23:59:35","No","No","No","Internal"]
[null,null,null,24518,null,"50_22/03/2022 17:01:54","2022-02-16T23:59:35","Observation","Ship Staff","Suptd. Insp.","Cleaning stay wires","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.4","Very High","","","Clean all stay wires for mast//fwd//aft//midship. Renew those which are wasted.\n- Cleaning & Greasing of Fwd mast,  Midhsip post, Mast riser Post, Light post near 2C & 5C completed. \nCleaning & Greasing of Aft mast stay  wires completed.","2022-10-10T23:59:35","","Completed","2022-09-28T23:59:35","No","No","No","Internal"]
[null,null,null,24519,null,"50_22/03/2022 17:45:23","2022-02-16T23:59:35","Observation","Ship Staff","Suptd. Insp.","Windlass gear engaging lever hydraulic assemblyto be cleaned, in bad shape.","Deck - Mooring Machinery","Mooring","Equipment Related","9.14","Medium","","","Cleaning of Both Windlass gear engaging leaver hyd. Assembly completed. Maintenance on Both windlass carried out.","2022-06-25T23:59:35","","Completed","2022-06-18T23:59:35","No","No","No","Internal"]
[null,null,null,24520,null,"50_22/03/2022 17:49:57","2022-02-16T23:59:35","Observation","Ship Staff","Suptd. Insp.","Both windlass leakage from blocks to be rectified.","Deck - Mooring Machinery","Mooring","Equipment Related","9.2","Very High","","","Port & Stbd windlass leaking block overhauled and fitted back. ","2022-06-25T23:59:35","","Completed","2022-06-18T23:59:35","No","No","No","Internal"]
[null,null,null,24524,null,"50_23/03/2022 04:36:28","2022-02-16T23:59:35","Observation","Ship Staff","Suptd. Insp.","Both Life boats de-rusting and greasing to be done.","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.28","Very High","","","Both Life Boat Davit de-rusted,painted and greasing of wires completed.","2022-03-16T23:59:35","","Completed","2022-03-07T23:59:35","No","No","No","Internal"]
[null,null,null,24525,null,"50_23/03/2022 04:42:35","2022-02-16T23:59:35","Observation","Ship Staff","Suptd. Insp.","Foam isolating valves to be greased and check for free movement.","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.38","High","","","All the foam & fire isolation valves on deck greased and freed. ","2022-04-16T23:59:35","","Completed","2022-03-15T23:59:35","No","No","No","Internal"]
[null,null,null,24526,null,"50_23/03/2022 04:46:38","2022-02-16T23:59:35","Observation","Ship Staff","Suptd. Insp.","Spot chipping and painting to be done - deck area.","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.3","Medium","","","Derusting & painting of deck fittings, Main deck area & mooring winch completed.","2022-12-10T23:59:35","","Completed","2022-11-30T23:59:35","No","No","No","Internal"]
[null,null,null,24527,null,"50_23/03/2022 04:54:21","2022-02-16T23:59:35","Observation","Ship Staff","Suptd. Insp.","funnel deck to be painted.","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.3","Medium","","","FUNNEL DECK, AESTHETIC APPEARANCE IS DULL, TO PAINT. \nSHIP’S STAFF COMMENTS: FUNNEL DECK, COAMING, EXHAUST PIPES DE-RUSTING AND PAINTING CARRIED OUT.\n","2022-10-10T23:59:35","","Completed","2022-10-10T23:59:35","No","No","No","Internal"]
[null,null,null,24528,null,"50_23/03/2022 05:38:00","2022-02-16T23:59:35","Observation","Ship Staff","Suptd. Insp.","Remove silicon and overhaul all PV valves","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.41","Medium","","","4P, 4S, 5P, 5S, 5C, Slop P & Slop S P.V valve have been overhauled and fitted back. 1, 2 & 3 arcoss & 4C PV valve overhauled after discharge port & fitted back. Almost all the PV valve still leaking, Sealed with silicon again in order to avoid loss of cargo vapour.","2022-06-25T23:59:35","","Completed","2022-05-12T23:59:35","No","No","No","Internal"]
[null,null,null,24529,null,"50_23/03/2022 05:42:31","2022-02-16T23:59:35","Observation","Ship Staff","Suptd. Insp.","Maintenance/de-rusting of super structure.","Accommodation","General Appearance","Equipment Related","11.8","Low","","","SUPER STRUCTURE HAS LOT OF RUST. NEED TO CLEAN WITH METAL BRITE AND CARRYOUT MAINTENANCE AS REQUIRED.\nSHIP’S STAFF COMMENTS: DERUSTING AND PAINTING OF ACCOMMODATION BLOCK CARRIED OUT.","2022-12-10T23:59:35","","Completed","2022-11-26T23:59:35","No","No","No","Internal"]
[null,null,null,24531,null,"50_23/03/2022 05:59:15","2022-02-16T23:59:35","Observation","Ship Staff","Suptd. Insp.","Cover for Valve hydraulic lines near dip tray to be fabricated and fitted with bolts ","Deck - Machinery","Cargo / Ballast Systems","Equipment Related","2.16","Medium","","","Cover for Valve hydraulic lines near dip tray fabricated and fitted with bolts.","2022-11-10T23:59:35","","Completed","2022-11-21T23:59:35","No","No","No","Internal"]
[null,null,null,24532,null,"50_23/03/2022 06:14:11","2022-02-16T23:59:35","Observation","Ship Staff","Suptd. Insp.","Sampling valves of COT handle are broken. ","Cargo Mach.,Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.22","Very High","","","Sampling valves of COT handle fixed in position.","2022-10-10T23:59:35","","Completed","2022-10-02T23:59:35","No","No","No","Internal"]
[null,null,null,24533,null,"50_23/03/2022 06:23:03","2022-02-16T23:59:35","Observation","Ship Staff","Suptd. Insp.","Dresser coupling - Paint removed from expansion area and grease applied.","Deck - Pipe / Fittings","General Appearance","Equipment Related","8.3","Very High","","","Removal of paint & greasing of dresser coupling carried out.","2022-10-10T23:59:35","","Completed","2022-09-28T23:59:35","No","No","No","Internal"]
[null,null,null,24534,null,"50_23/03/2022 06:27:49","2022-02-16T23:59:35","Observation","Ship Staff","Suptd. Insp.","PV breaker/ Mast raiser Breather valve looks to be blanked. SA investigated ","Cargo Mach.,Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.36","Medium","","","Mast riser breather valve inspected,cleaned and fitted back.No blank found.","2022-04-16T23:59:35","","Completed","2022-05-08T23:59:35","No","No","No","Internal"]
[null,null,null,24536,null,"50_23/03/2022 06:38:51","2022-02-16T23:59:35","Observation","Ship Staff","Suptd. Insp.","ER Skylight de-rusting and paint. ","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.6","Medium","","","ER Skylight De-rusted and painted.","2022-05-25T23:59:35","","Completed","2022-05-11T23:59:35","No","No","No","Internal"]
[null,null,null,24537,null,"50_23/03/2022 04:58:16","2022-02-16T23:59:35","Observation","Ship Staff","Suptd. Insp.","Limit switch on Port mid-ship crane to be repaired.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.5","Very High","","","Replaced with supplied spares, tried out and found working satisfactory.","2022-05-12T23:59:35","DPEO 220095","Completed","2022-03-20T23:59:35","No","No","No","Internal"]
[null,null,null,24538,null,"50_23/03/2022 07:17:30","2022-02-16T23:59:35","Observation","Ship Staff","Suptd. Insp.","Inspect portable lifting gear and damaged gears to be discarded.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.28","Low","","","Damaged lifting gears discarded.","2022-04-25T23:59:35","","Completed","2022-04-21T23:59:35","No","No","No","Internal"]
[null,null,null,24539,null,"50_23/03/2022 07:23:58","2022-02-16T23:59:35","Observation","Ship Staff","Suptd. Insp.","MAC no # 3 is not operational","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","CRANKSHAFT,MAIN BEARING AND BOTTOM END BEARING SHELL  RENEWED , TRIED OUT FOUND SATISFACTORY","2022-12-25T23:59:35","DPEO220027","Completed","2022-12-29T23:59:35","No","No","No","Internal"]
[null,null,null,24540,null,"50_23/03/2022 16:38:32","2022-02-16T23:59:35","Observation","Ship Staff","Suptd. Insp.","Inventory of spares to be taken","Documentation","Eng. / Strg. Comp.","Equipment Related","10.12","Very High","","","Spare inventory  updated in PAL. ","2022-04-25T23:59:35","","Completed","2022-04-21T23:59:35","No","No","No","Internal"]
[null,null,null,24541,null,"50_23/03/2022 16:49:11","2022-02-16T23:59:35","Observation","Ship Staff","Suptd. Insp.","Ballast pump No 1 to be made operational. ","Deck - Machinery","Cargo / Ballast Systems","Equipment Related","8.19","High","","","Bearing failure and bearing top cover deformed due to heat. Same machined, bearing and mech seal replaced. Tried out. Working satisfactory. Spares received.  Pump has been in operation since last 4 months.  The pump valves need to be overhauled as leaking. ","2022-06-25T23:59:35","DPEO220124","Completed","2022-03-26T23:59:35","No","No","No","Internal"]
[null,null,null,24542,null,"50_23/03/2022 17:24:56","2022-02-16T23:59:35","Observation","Ship Staff","Suptd. Insp.","BWTS filters to clean and make operational","Deck - Machinery","Cargo / Ballast Systems","Equipment Related","6.21","High","","","BOTH BWTS FILTER CLEANING COMPLETED.","2022-06-18T23:59:35","","Completed","2022-05-22T23:59:35","No","No","No","Internal"]
[null,null,null,24543,null,"50_23/03/2022 18:19:48","2022-02-16T23:59:35","Observation","Ship Staff","Suptd. Insp.","Inspect gauges for correct operation.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","MDO SETTLING AND SERVICE TANK GAUGES renewed with newly received gauge. Leved confirmed with actual sounding. \n\n\n","2022-07-26T23:59:35","DPEO 220018","Completed","2022-07-20T23:59:35","No","No","No","Internal"]
[null,null,null,24546,null,"50_23/03/2022 18:29:24","2022-02-16T23:59:35","Observation","Ship Staff","Suptd. Insp.","Check M/E F.O. Module steam controller.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","M/E F.O. MODULE STEAM CONTROLLER NOT WORKING PROPERLY AS PER THE COMMAND. Same working good.\n\n\n\n","2022-07-26T23:59:35","","Completed","2022-06-09T23:59:35","No","No","No","Internal"]
[null,null,null,24547,null,"50_23/03/2022 07:11:27","2022-02-16T23:59:35","Observation","Ship Staff","Suptd. Insp.","Soft patch on IG deck NRV OD valve. ","Inert Gas","Eng. / Strg. Comp.","Equipment Related","8.31","High","","","Soft patch on IG deck NRV OD valve. \n- Observation entered wrongly, No soft patch on IG deck NRV OD valve. \n   Kindly advised weather vessel can delete this defect from DDRL.","2022-11-10T23:59:35","","Completed","2022-10-27T23:59:35","No","No","No","Internal"]
[null,null,null,24549,null,"50_23/03/2022 18:35:15","2022-02-16T23:59:35","Observation","Ship Staff","Suptd. Insp.","Inspect SOX airvent pot leakage.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","SOX WMS-002 AIRVENT POT LEAKING FROM THE AIR AUTO RELEASE VENT. REPLACED.\n\n\n\n","2022-06-25T23:59:35","DPEO 220042","Completed","2022-05-23T23:59:35","No","No","No","Internal"]
[null,null,null,24550,null,"50_23/03/2022 18:37:32","2022-02-16T23:59:35","Observation","Ship Staff","Suptd. Insp.","SOX PAH sensor reading to calibrate.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","SOX WMS-002 PAH SENSOR CALIBRATION CARRIED OUT WITH ZERO REFERENCE LIQUID. NOW PAH SENSOR READING IS WITHIN LIMITS\n\n","2022-05-12T23:59:35","DPEO 220031","Completed","2022-04-11T23:59:35","No","No","No","Internal"]
[null,null,null,24551,null,"50_23/03/2022 18:41:04","2022-02-16T23:59:35","Observation","Ship Staff","Suptd. Insp.","Inspect and replace cabinet.","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.4","High","","","NEW CO2 CABINET INSTALLED IN FIRE STATION AT MINA AL FAHAL ANCHORAGE","2022-08-26T23:59:35","DPEO 220139","Completed","2022-07-28T23:59:35","No","No","No","Internal"]
[null,null,null,24552,null,"50_23/03/2022 18:45:22","2022-02-16T23:59:35","Observation","Ship Staff","Suptd. Insp.","Inspect M/eng unit no.1 Jacket water leak.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Lover quill overhauled and replaced O rings and gaskets. No leaks.\n\n\n\n","2022-05-16T23:59:35","","Completed","2022-03-29T23:59:35","No","No","No","Internal"]
[null,null,null,24553,null,"50_23/03/2022 18:58:07","2022-02-16T23:59:35","Observation","Ship Staff","Suptd. Insp.","Check deck scuppers for leaks. Raise requisiton for proper size scuppers.","Deck - Pipe / Fittings","MARPOL Related","Equipment Related","6.2","High","","","25 NO'S SCUPPER PLUG RECEIVED ON 18/07/2022 @ SINGAPORE","2022-08-10T23:59:35","","Completed","2022-07-13T23:59:35","No","No","No","Internal"]
[null,null,null,24554,null,"50_23/03/2022 19:36:15","2022-02-16T23:59:35","Observation","Ship Staff","Suptd. Insp.","AE backwash filter to be inspected for proper operation.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Working satisfactory.\n\n\n\n","2022-05-26T23:59:35","","Completed","2022-05-20T23:59:35","No","No","No","Internal"]
[null,null,null,24555,null,"50_23/03/2022 19:41:47","2022-02-16T23:59:35","Observation","Ship Staff","Suptd. Insp.","Inspect meat room temperature sensor irrating reading","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Meat room temperature renewed with newly received sensor. Found working satisfactory.\n\n\n\n","2022-07-20T23:59:35","DPEO220133","Completed","2022-07-23T23:59:35","No","No","No","Internal"]
[null,null,null,24556,null,"50_23/03/2022 19:45:28","2022-02-16T23:59:35","Observation","Ship Staff","Ship Staff Insp.","WMS-002 Pump capacitor burning during start of plant","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","The pump is now started after 10 to 15 minutes of system start up. Initial soot particles is more, and was effective the performance.  For last 3 months there has been no issue with the pump.\n\n\n\n","2022-05-16T23:59:35","","Completed","2022-05-15T23:59:35","No","No","No","Internal"]
[null,null,null,24558,null,"50_22/03/2022 16:26:59","2022-02-16T23:59:35","Observation","Ship Staff","Suptd. Insp.","Port windlass Bearing to renew","Deck - Mooring Machinery","Mooring","Equipment Related","9.2","Very High","","","Port Anchor windlass port centre and free end half bearing bush renewed.Centre bearing upper half bearing bush holes were not matching with holding screw of housing. So new holes made in the shell and other holes blinded. Windlass tried out. No wobbling in the shaft","2022-03-16T23:59:35","","Completed","2022-02-19T23:59:35","No","No","No","Internal"]
[null,null,null,24559,null,"50_22/03/2022 18:27:26","2022-02-16T23:59:35","Observation","Ship Staff","Suptd. Insp.","Pedestal rollers to be de-rusted and made free for movement.","Deck - Mooring Machinery","General Appearance","Equipment Related","9.18","Low","","","All Roller’s removed from place Cleaned,De-rusted, painted and fitted back.Moving freely.","2022-05-16T23:59:35","","Completed","2022-03-01T23:59:35","No","No","No","Internal"]
[null,null,null,24560,null,"50_23/03/2022 05:51:01","2022-02-16T23:59:35","Observation","Ship Staff","Suptd. Insp.","Port side Drip tray under manifold need maintenance. ","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.67","High","","","Soft repair done on base support and painted. To be included in REFMAN. ","2022-04-16T23:59:35","","Completed","2022-02-21T23:59:35","No","No","No","Internal"]
[null,null,null,24561,null,"50_23/03/2022 06:18:49","2022-02-16T23:59:35","Observation","Ship Staff","Suptd. Insp.","Deck seal steam line to be renewed","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.4","Very High","","","IG deck seal steam line pipe removed and renewed,painted and fitted back.","2022-05-16T23:59:35","","Completed","2022-03-14T23:59:35","No","No","No","Internal"]
[null,null,null,24562,null,"50_23/03/2022 16:36:23","2022-02-16T23:59:35","Observation","Ship Staff","Suptd. Insp.","Check and filing of Analysis report and test in file.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.7","Medium","","","On board LO Analysis docs are not filled. Drop test data not available. Same started from Feb 2022","2022-03-05T23:59:35","","Completed","2022-02-16T23:59:35","No","No","No","Internal"]
[null,null,null,24563,null,"50_23/03/2022 17:30:15","2022-02-16T23:59:35","Observation","Ship Staff","Suptd. Insp.","Elevator auto-closer doors closing sped to be adjusted.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Lift doors at each floor are very fast, need to adjust auto closer. \n\nSame done by Service Engineer at Fujairah.\n\n","2022-03-16T23:59:35","","Completed","2022-03-01T23:59:35","No","No","No","Internal"]
[null,null,null,24564,null,"50_23/03/2022 16:28:49","2022-02-16T23:59:35","Observation","Ship Staff","Suptd. Insp.","STP pipe to clean and made operational.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","STP all chamber cleaned from inside . sludge deposits removed from the bottom. After box back STp tried out. Working satisfactory","2022-04-16T23:59:35","","Completed","2022-02-17T23:59:35","No","No","No","Internal"]
[null,null,null,24565,null,"50_23/03/2022 07:29:35","2022-02-16T23:59:35","Observation","Ship Staff","Suptd. Insp.","OWS OVBD flanges are with only one seal per flange. 2 seals to be put.","Critical Equip.","Eng. / Strg. Comp.","Equipment Related","6.16","Very High","","","OWS OVBD flanges were with only one seal per flange. 2 seals has been put and form is updated. ","2022-03-16T23:59:35","","Completed","2022-03-21T23:59:35","No","No","No","Internal"]
[null,null,null,24557,null,"50_27/03/2022 21:03:38","2022-03-21T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Oxygen gas cylinder bottle and line both flash back arrestors will expire in Mar 2022","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","5.27","Medium","","","Both flash back arrestors renewed","2022-06-25T23:59:35","","Completed",null,"No","No","No","Internal"]
[null,null,null,26106,70066,"0_Mon May 09 2022 13:43:56 GMT+0800","2022-04-30T23:59:35","Observation","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","Discrepancies noted in filling of enclosed space entry permit checklist.","Documentation","ISM Related","Human Error","5.16","Very High","","","Permit was correctly filled, however as the permit was maintained at the work site and was soiled by working hands of the Responsible officer, the uploaded permits for the remote SIRE were duplicate clean copy albeit with missed entries. This was a clerical error.","2022-06-25T23:59:35","","Completed","2022-04-30T23:59:35","No","No","No","External"]
[null,null,null,26107,54084,"50_Mon May 09 2022 13:39:54 GMT+0800","2022-04-30T23:59:35","Observation","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","Records of work and rest hour for the month of April was not updated effectively in the documents provided.","Documentation","Crew Management","Human Error","3.2","Very High","","","Uploaded Rest hours was incomplete as Month of April was not complete. EOM April Rest hours was completed and presented to inspector at time of inspection on 5/May 2022","2022-06-25T23:59:35","","Completed","2022-04-30T23:59:35","No","No","No","External"]
[null,null,null,26108,44024,"0_Mon May 09 2022 13:46:34 GMT+0800","2022-05-01T23:59:35","Observation","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","HFO & MGO pressure test certificate was having difference in test pressure and rating pressure. ","Documentation","ISM Related","Human Error","6.7","High","","","Test certificate pressure rating amended.","2022-06-25T23:59:35","","Completed","2022-05-16T23:59:35","No","No","No","External"]
[null,null,null,26109,87596,"50_Thu Jun 30 2022 17:15:20 GMT+0800","2022-05-10T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","AE # 2: LO auto back wash filter element bearing failure. ","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Put in service as not effecting the operations.\nSpares received on 29/June/2022. \nJob carried out and replaced the bearings. Working satisfactory.","2022-07-10T23:59:35","DPEO220192","Completed","2022-06-26T23:59:35","No","No","No","Internal"]
[null,null,null,26098,79875,"50_Sun Jun 26 2022 10:35:12 GMT+0800","2022-05-13T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Following valves leaking and needs to be replaced.\n1. Vacuum condensor SW in/out valves -2\n2.Aux boiler feed pumps return - 2\n3. Aux boiler feed pump discharge valves both pumps - 2\n4. HP circ pump discharge valve -2\n5. Primary bilge tank & ME JCW buffer tank valve -2","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Following valve renewed with newly received one.\n1. Vacuum condenser Air ejector S/W IN / OUT valve\n5. Primary bilge tank valve replaced.\n6. ME JCW buffer tank valve\nFor other valves, awaiting for suitable opertunity.","2022-11-25T23:59:35","DPEO5080","Completed","2022-09-09T23:59:35","No","No","No","Internal"]
[null,null,null,26102,61436,"50_Mon Jun 27 2022 10:25:21 GMT+0800","2022-05-13T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Low Sea Chest suction strainer inlet valve - very hard to operate although the valves are holding for routine cleaning of filter","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Valve gear machenism removed from place.  Valve spindle found to stuck with gear housing cover.  Same eased up. All parts de rusted and cleaned. Fitted back in place. greasing of rotating machenisam done. Valve smooth operatipn confirmed.","2022-07-26T23:59:35","","Completed","2022-07-10T23:59:35","No","No","No","Internal"]
[null,null,null,26101,35926,"50_Sun Jun 26 2022 11:32:33 GMT+0800","2022-06-04T23:59:35","Defect","Ship Staff","Ship Staff Insp.","AE # 1: Turbocharger water washing line (one section defective). ","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","T/C WATER WASHING LINE FITTED AND TRIED OUT FOUND SATISFACTORY","2022-12-26T23:59:35","DPEO220164","Completed","2022-12-18T23:59:35","No","No","No","Internal"]
[null,null,null,26103,38185,"50_Mon Jun 27 2022 11:04:48 GMT+0800","2022-06-05T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Steam pressure 4k relief valve: Same was overhauled ashore but still leaking","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Renewed from spare.","2023-05-26T23:59:35","DPEO230013","Completed","2023-06-06T23:59:35","No","No","No","Internal"]
[null,null,null,26110,78985,"50_Sun Jun 26 2022 11:38:24 GMT+0800","2022-06-05T23:59:35","Defect","Ship Staff","Ship Staff Insp.","7K steam pneumatic positioner defective. To be replaced.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Requisition made. Spares received. \nFitted and put in service. Working satisfactory.","2022-07-10T23:59:35","DPEO225089","Completed","2022-06-26T23:59:35","No","No","No","Internal"]
[null,null,null,29487,91741,"50_Wed Mar 08 2023 10:42:18 GMT+0800","2022-06-06T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Nav Audit / Verification","One OOW did not know the use of RAPTOR","Navigation - Others","Navigation","Knowledge Based","","","","","Training given to O.O.W and explained the function of RAPTOR","2022-07-06T23:59:35","","Completed","2022-06-08T23:59:35","No","No","No","Internal"]
[null,null,null,29488,62661,"50_Wed Mar 08 2023 10:44:56 GMT+0800","2022-06-06T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Nav Audit / Verification","Log book entry on 3rd was not completed by one OOW.","Navigation - Others","Navigation","Human Error","","","","","O.O.W. was called immediately and asked to complete the log book entry","2022-07-06T23:59:35","","Completed","2022-06-08T23:59:35","No","No","No","Internal"]
[null,null,null,26104,84846,"50_Fri Jul 01 2022 09:22:53 GMT+0800","2022-06-09T23:59:35","Defect","Ship Staff","Ship Staff Insp.","AE # 2: JCW inlet valve not holding & leaking. Running time no issue. Problem during overhaul routines.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Leaking valve eased up. Gland lubricated. Valve shut and checked for any leaks. Found valve holdind. ","2022-07-26T23:59:35","DPEO220208","Completed","2022-07-19T23:59:35","No","No","No","Internal"]
[null,null,null,26105,46926,"50_Fri Jul 01 2022 10:31:22 GMT+0800","2022-06-11T23:59:35","Defect","Ship Staff","Ship Staff Insp.","BALLAST PUMP MOTOR #1 MCCB 800A  SUPPLY INCOMING STRIP GETTING HOT BECAUSE SECURING SCREW SLIGHTLY LOOSE.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.8","Medium","","","Renewed and observed working satisfactorily.","2023-04-25T23:59:35","DPEO220203","Completed","2023-03-31T23:59:35","No","No","No","Internal"]
[null,null,null,26100,40334,"50_Sun Jun 26 2022 11:10:44 GMT+0800","2022-06-16T23:59:35","Defect","Ship Staff","Ship Staff Insp.","ME JCW filling valve leaking","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Valev replace with newly received spare valve. Valve opertaion confirmed. No further leaksgs.","2022-08-26T23:59:35","DPEO220208","Completed","2022-07-27T23:59:35","No","No","No","Internal"]
[null,null,null,26099,67607,"50_Sun Jun 26 2022 11:05:10 GMT+0800","2022-06-17T23:59:35","Defect","Ship Staff","Ship Staff Insp.","FWG: Ejector pump discharge valve to be replaced as has pin hole in casing","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Valve replace with newly received valve. All gasket remewed. Pump tried out. No leaks.","2022-07-26T23:59:35","DPEO220208","Completed","2022-07-15T23:59:35","No","No","No","Internal"]
[null,null,null,26111,77747,"50_Wed Jul 06 2022 09:02:52 GMT+0800","2022-06-23T23:59:35","Defect","Ship Staff","Ship Staff Insp.","ME JCW pre heater steam valve leak.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Same replaced.","2022-07-08T23:59:35","","Completed","2022-06-29T23:59:35","No","No","No","Internal"]
[null,null,null,27396,77965,"50_Sun Oct 02 2022 20:22:30 GMT+0800","2022-07-14T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Stbd manifold drip tray grating not secured with clamps","Cargo Mach.","Cargo / Ballast Systems","Human Error","8.67","High","","","Stbd manifold drip tray grating secured with clamps.\n","2022-10-15T23:59:35","","Completed","2022-09-26T23:59:35","No","No","No","Internal"]
[null,null,null,27397,10643,"50_Sun Oct 02 2022 20:10:38 GMT+0800","2022-07-14T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Dump valve instructions/warnings faded","Cargo Mach.","Cargo / Ballast Systems","Human Error","6.3","Low","","","Dump valve instructions/warnings stenciled.","2022-10-15T23:59:35","","Completed","2022-07-05T23:59:35","No","No","No","Internal"]
[null,null,null,27398,55920,"0_Sun Oct 02 2022 16:15:42 GMT+0800","2022-07-14T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Foundation of wilden pump kept on stbd break of accomodation found corroded","Cargo Mach.","","Equipment Related","6.3","Low","","","Foundation of wilden pump kept on stbd/port break of accommodation derusted and painted.","2022-10-14T23:59:35","","Completed","2022-09-29T23:59:35","No","No","No","Internal"]
[null,null,null,27399,43685,"50_Sun Oct 02 2022 20:19:14 GMT+0800","2022-07-14T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","FW valve near stbd break of accomodation on upper deck leaking.","Deck - Pipe / Fittings","General Appearance","Equipment Related","10.32","Very High","","","FW valve near stbd break of accommodation on upper deck overhauled and refitted, found not leaking .","2022-10-15T23:59:35","","Completed","2022-09-30T23:59:35","No","No","No","Internal"]
[null,null,null,27401,95333,"50_Sun Oct 02 2022 20:40:11 GMT+0800","2022-07-14T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Vapour reducer kept in port midship store is painted orange instead of standard color code as per OCIMF requirement","Deck - Pipe / Fittings","Cargo / Ballast Systems","Inappropriate Procedure","8.42","Medium","","","Vapour reducer kept in port midship store is painted as per standard color code as per OCIMF requirement","2022-10-15T23:59:35","","Completed","2022-09-29T23:59:35","No","No","No","Internal"]
[null,null,null,27404,88309,"50_Sun Oct 02 2022 15:56:14 GMT+0800","2022-07-14T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Light fittings around acommodation developing rust","Elect. Mach. & Equip.","General Appearance","Equipment Related","","","","","light fittings which were rusted has been removed repaired or renewed in all places and also the base for the fittings has been renewed around thew acommodation and in the bridge wings all are in good condition now.","2022-12-25T23:59:35","","Completed","2022-12-03T23:59:35","No","No","No","Internal"]
[null,null,null,27423,12655,"50_Sun Oct 02 2022 21:19:43 GMT+0800","2022-07-14T23:59:35","Observation","Ship Staff","Suptd. Insp.","Reefer chambers call alarm log in the galley was last updated in December 2021. Is the inspection being carried out as per PMS","Accommodation","Safety / LSA / FFA","Human Error","11.13","Low","","","Reefer chambers call  testing and inspection  carried out weekly, updated from october 2022 onward","2022-10-15T23:59:35","","Completed","2022-09-26T23:59:35","No","No","No","Internal"]
[null,null,null,27432,32459,"50_Sun Oct 02 2022 21:34:28 GMT+0800","2022-07-14T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Several MSDS for chemicals were found to be very old and needs to be updated with new versions.","Documentation","Cert. & Docu.","Inappropriate Procedure","5.46","Medium","","","Old MSDS been renewed with new versions","2022-10-15T23:59:35","","Completed","2022-09-15T23:59:35","No","No","No","Internal"]
[null,null,null,27434,14161,"50_Sun Oct 02 2022 21:29:33 GMT+0800","2022-07-14T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","The crew change room was found very messy and winter gear was found all stuffed in lockers","Accommodation","MLC Related","Behaviour Based","11.14","Medium","","","The crew change room was cleaned and arranged. All lockers were cleaned and properly arranged.","2022-10-15T23:59:35","","Completed","2022-07-18T23:59:35","No","No","No","Internal"]
[null,null,null,27438,22123,"50_Sun Oct 02 2022 21:23:02 GMT+0800","2022-07-14T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","The oven in the galley was found to be in dirty condition with a lot of oil accumulated on the floor","Accommodation","General Appearance","Behaviour Based","11.13","Low","","","The oven in the galley was cleaned with no trace of oil deposit on the floor.","2022-10-15T23:59:35","","Completed","2022-07-16T23:59:35","No","No","No","Internal"]
[null,null,null,27439,28132,"50_Sun Oct 02 2022 21:26:21 GMT+0800","2022-07-14T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Knives in the galley were not found color coded and galley fridge food management was as not per MLC","Accommodation","MLC Related","Inappropriate Procedure","11.13","Low","","","Knives in the galley were color coded and galley fridge was arranged properly. ","2022-10-15T23:59:35","","Completed","2022-07-17T23:59:35","No","No","No","Internal"]
[null,null,null,27442,78919,"50_Wed Aug 24 2022 17:33:39 GMT+0800","2022-07-21T23:59:35","Defect","Ship Staff","Ship Staff Insp.","LT Cooler#1 S/W inlet pipe section fond to be leaking","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Cooler leaking section renewed with new fabricated section. After tightning, leak test carried out. No leaks observed. LT Cooler put back in use.","2022-08-26T23:59:35","","Completed","2022-07-26T23:59:35","No","No","No","Internal"]
[null,null,null,27392,81341,"50_Sat Sep 17 2022 12:43:53 GMT+0800","2022-08-04T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Main SW pp # 2 suction pipe leakage due to corrosion in main SW line from sea chest connection pipe., no isolation valve provided in the section.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.20","High","","","SW pp # 2 suction pipe wasted stub piece renewed with fabricated new pipe, ","2022-11-18T23:59:35","","Completed","2022-11-14T23:59:35","No","No","No","Internal"]
[null,null,null,27394,33084,"50_Mon Aug 22 2022 18:37:17 GMT+0800","2022-08-05T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Hot water calofier two heater found not working and giving 440V low insulation.","","Eng. / Strg. Comp.","External Factors","","","","","HOT WATER CALORIFIER OPENED UP CLEANED AND HEATER RENEWED WITH NEW ONE.","2022-12-26T23:59:35","DPEO220222","Completed","2023-01-02T23:59:35","No","No","No","Internal"]
[null,null,null,27441,24145,"50_Wed Aug 24 2022 17:21:06 GMT+0800","2022-08-05T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Elevator door closing operation found sluggish.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Elevator Door belt found to be damaged. same renewed. Greasing of bearing carried out. Door operation checked. found smooth.","2022-08-26T23:59:35","","Completed","2022-08-09T23:59:35","No","No","No","Internal"]
[null,null,null,27391,25593,"50_Wed Aug 24 2022 17:45:52 GMT+0800","2022-08-05T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","HP Circulating Pump has abnormal vibration and discharge pressure found to be low.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","NEW PUMP INSTALLED AND TRIED OUT FOUND WORKING SATISFACTORY.","2022-12-26T23:59:35","DPEO220222","Completed","2022-12-21T23:59:35","No","No","No","Internal"]
[null,null,null,23728,null,"50_15/01/2022 4:00:27 PM","2022-08-07T23:59:35","Defect","Ship Staff","Ship Staff Insp.","AE NO.1 Air cooler four tubes found leaking same being blanked.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","AE No:1 air cooler renewed with spare new one. ","2023-01-26T23:59:35","DPEO220014","Completed","2023-02-10T23:59:35","No","No","No","Internal","spares ordered, awaiting readiness."]
[null,null,null,27395,76633,"50_Sat Sep 17 2022 16:40:38 GMT+0800","2022-08-12T23:59:35","Observation","Ship Staff","Ship Staff Insp.","DECK HYDRAULICS, TEMPERATURE SWITCH COVER FOUND BROKEN.","Deck - Mooring Machinery","General Appearance","External Factors","9.15","Medium","","","REQUISTION WAS CANCELLED FROM OFFICE. THE BROKEN SWITCH COVER WAS COVERED WITH FABRICATED ACRYLIC BOX.","2022-12-25T23:59:35","DPEO220240","Completed","2023-02-15T23:59:35","No","No","No","Internal"]
[null,null,null,27424,51964,"50_Tue Aug 30 2022 07:48:17 GMT+0800","2022-08-22T23:59:35","Defect","Ship Staff","Suptd. Insp.","FWG distillate recirculation line solenoid valve not operating at high PPM.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","FWG distillate recirculation line Solenoid valve removed from place. Diaphragm found to be damaged. Solenoid valve replaced with new one. Solenoid valve operation checked, found to be working satisfactory.","2022-08-26T23:59:35","","Completed","2022-08-24T23:59:35","No","No","No","Internal"]
[null,null,null,27425,51263,"50_Tue Sep 06 2022 14:20:40 GMT+0800","2022-08-25T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Aux. Boiler#1 circulating line secondary valve bonnet and valve flange found to be leaking. Same to be rectify.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Aux. Boiler#1 isolated. Circulating line secondary valve bonnet and flange gasket renewed. All bolts greased. After tightning, leak test carried out. No further leakage.","2022-09-10T23:59:35","","Completed","2022-08-30T23:59:35","No","No","No","Internal"]
[null,null,null,27431,47221,"50_Fri Sep 16 2022 22:15:54 GMT+0800","2022-08-27T23:59:35","Observation","Ship Staff","Ship Staff Insp.","LT Cooler S/W inlet and outlet pipe section found to be leaking","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Both pipe section renewed with assistance of shore contractor.  At present there is no leaks. ","2022-09-11T23:59:35","","Completed","2022-09-09T23:59:35","No","No","No","Internal"]
[null,null,null,27420,79762,"50_Mon Oct 03 2022 13:07:39 GMT+0800","2022-08-28T23:59:35","Observation","Ship Staff","Ship Staff Insp.","OWS  Oil sensor defective and not giving output to Oil valve  to open to waste oil tank , ","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","RECEIVED NEW OIL SENSOR AND FITTED IN PLACE AND TESTED, OPERATION CHECKED AND WORKING SATISFACTORY.","2023-01-12T23:59:35","DPEO 220268 - OIL LEVEL SENSOR FOR OWS","Completed","2022-12-08T23:59:35","No","No","No","Internal"]
[null,null,null,27427,82731,"50_Fri Sep 16 2022 22:04:09 GMT+0800","2022-09-05T23:59:35","Defect","Ship Staff","Ship Staff Insp.","LO Purifier #2 Feed pump got overload trip.","E/R - Aux. Mach.","","Equipment Related","10.32","Very High","","","Motor removed from place. Found hard to turm. Motor dismentled. Found NDE bearing hard to rotate. Both bearing for the  motor renewed. Motor assembled back. Insulation test carried out. Found infinity. Motor fitted back in place and tried out. Working fine.","2022-09-25T23:59:35","","Completed","2022-09-11T23:59:35","No","No","No","Internal"]
[null,null,null,27428,79205,"50_Fri Sep 16 2022 21:58:59 GMT+0800","2022-09-05T23:59:35","Defect","Ship Staff","Ship Staff Insp.","AE#3 unit 6 and 7 exhaust temperature reading irratic.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","unit # 6 & 7 temperature sensor renewed with new one","2022-10-26T23:59:35","","Completed","2022-09-15T23:59:35","No","No","No","Internal"]
[null,null,null,27426,58325,"50_Fri Sep 16 2022 21:55:09 GMT+0800","2022-09-07T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Aux Boiler Aux feed water Pump motor tripped on overload","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Motor inspected. Found hard to rotate. Same motor removed from place and overhauled. DE bearing found to be jammed due to overheating. Both end bearing renewed. Motor fitted back in place. Pump tried out. Working fine.","2022-09-15T23:59:35","","Completed","2022-09-10T23:59:35","No","No","No","Internal"]
[null,null,null,27393,27169,"50_Fri Sep 16 2022 22:12:23 GMT+0800","2022-09-08T23:59:35","Observation","Ship Staff","Ship Staff Insp.","OWS 15 PPM monitor got hanged some time when in operation.","Critical Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Tried out operation of the OWS for emptying both bilge holding tank and clean drain tank. Presently working in good order without any trouble.","2023-01-26T23:59:35","DPEO220288","Completed","2023-02-01T23:59:35","No","No","No","Internal"]
[null,null,null,24530,null,"50_23/03/2022 05:46:33","2022-09-14T23:59:35","Observation","Ship Staff","Suptd. Insp.","Cranes-. Derusting and greasing to be carried out. ","Cargo Mach.,Deck - Machinery","General Appearance","Equipment Related","8.5","Very High","","","COMPLETED DERUSTING & PAINTING OF PORT/STBD HHC COMPLETED.\nGREASING OF ALL CRANES CARRIED OUT.","2023-01-25T23:59:35","","Completed","2023-01-25T23:59:35","No","No","No","Internal"]
[null,null,null,27405,98293,"0_Sun Oct 02 2022 23:41:33 GMT+0800","2022-09-15T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Isolation valve for all Mooring Winches found very hard. All valves to be freed up and ensure they are moving freely. ","Deck - Mooring Machinery","Mooring","Equipment Related","9.4","High","","","Isolation valve for all Mooring Winches freed up for free movement.","2022-10-15T23:59:35","","Completed","2022-09-30T23:59:35","No","No","No","Internal"]
[null,null,null,27406,72411,"0_Sun Oct 02 2022 23:43:01 GMT+0800","2022-09-15T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Starboard Windlass brake cylinder oil seal found leaking. Same is to be renewed","Deck - Mooring Machinery","Mooring","Equipment Related","9.2","Very High","","","Oil seal renewed and leak rectified.","2023-01-26T23:59:35","DPEO220160","Completed","2023-02-11T23:59:35","No","No","No","Internal"]
[null,null,null,27407,84304,"0_Sun Oct 02 2022 23:44:34 GMT+0800","2022-09-15T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Port windlass few hydraulic hose found in bad condition. Vessel has spare hoses and same is to be renewed asap. ","Deck - Mooring Machinery","Mooring","Equipment Related","9.2","Very High","","","R.O. DPEO2201311  has been raised for the spare hoses as the hoses onboard is short in length, other hoses has been renewed","2023-02-10T23:59:35","DPEO220311","Completed","2023-02-24T23:59:35","No","No","No","Internal"]
[null,null,null,27408,53065,"0_Sun Oct 02 2022 23:50:07 GMT+0800","2022-09-15T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","FW line to deck found rusted and corroded. Several sections needs to be immediately renewed","Deck - Pipe / Fittings,Hull & Tanks","Structural Condn. / WT integrity ","Behaviour Based","11.4","Very High","","","FW line to deck to be derusted and painted.","2022-12-15T23:59:35","","Completed","2022-10-18T23:59:35","No","No","No","Internal"]
[null,null,null,27409,73642,"50_Mon Oct 03 2022 00:48:37 GMT+0800","2022-09-15T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Floor plate near ME Cylinder head no 1 found vibrating excessively. Same needs to be arrested. Additional clamping arrangement would be required","Miscellaneous","Eng. / Strg. Comp.","Knowledge Based","10.32","Very High","","","Floor plates were screwed and and additional clamping arrangement made","2022-11-05T23:59:35","","Completed","2022-11-04T23:59:35","No","No","No","Internal"]
[null,null,null,27410,39508,"0_Sun Oct 02 2022 23:46:45 GMT+0800","2022-09-15T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","F-spanners found missing at several fire hydrants. All fire hydrants to have one dedicated F spanner","LSA / FFA","Safety / LSA / FFA","Knowledge Based","12.15","High","","","F-spanners to be placed to all fire hydrants","2022-10-15T23:59:35","","Completed","2022-09-28T23:59:35","No","No","No","Internal"]
[null,null,null,27411,90762,"50_Sun Oct 02 2022 23:27:37 GMT+0800","2022-09-15T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Class approved Fuel Oil change over procedure could not be located. Same is to be posted in the ER and all Engineers should be familiar with the procedure","Documentation","Eng. / Strg. Comp.","Knowledge Based","10.9","Medium","","","Class approved Fuel change over procedure kept in ECR","2022-12-25T23:59:35","","Completed","2022-10-29T23:59:35","No","No","No","Internal"]
[null,null,null,27412,40202,"0_Mon Oct 03 2022 00:54:08 GMT+0800","2022-09-15T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","All fire sensors to be identified and marked below the sensor for ease of identification. ","LSA / FFA","Safety / LSA / FFA","Knowledge Based","5.35","Medium","","","All sensor markings has been carried out, for identification.","2022-11-15T23:59:35","","Completed","2022-11-07T23:59:35","No","No","No","Internal"]
[null,null,null,27413,83081,"0_Mon Oct 03 2022 00:57:22 GMT+0800","2022-09-15T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","40 ltrs Foam extinguisher on ECR Platform (near Port Aux Boiler) found secured by metal wire. This should be of quick release type. ","LSA / FFA","Safety / LSA / FFA","Knowledge Based","12.15","High","","","New quick release clamp fabricated and secured the foam extinguisher","2022-10-15T23:59:35","","Completed","2022-10-01T23:59:35","No","No","No","Internal"]
[null,null,null,27415,66675,"0_Mon Oct 03 2022 01:02:51 GMT+0800","2022-09-15T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Vent head on the funnel platform found rusted and wire mesh cover found missing. Same to be overhauled and repaired","","","","11.7","High","","","Vent head removed from place, wire mesh and cover new one fabricated all rusts removed and primer applied .\nBoth vent head assembled  and fitted back.","2022-10-15T23:59:35","","Completed","2022-10-06T23:59:35","No","No","No","Internal"]
[null,null,null,27416,90308,"0_Mon Oct 03 2022 01:20:11 GMT+0800","2022-09-15T23:59:35","Non Conformity","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Engineers found not maintaining Individual handwritten daily work done book as per official circular issued by Office. ","Documentation","Cert. & Docu.","Knowledge Based","2.3","High","","","All engineers  have started to use the daily work done note book","2022-10-10T23:59:35","","Completed","2022-09-16T23:59:35","No","No","No","Internal"]
[null,null,null,27419,20456,"0_Mon Oct 03 2022 00:59:03 GMT+0800","2022-09-15T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Main Funnel stack needs immediate de-rusting and painting","Hull & Tanks","General Appearance","Behaviour Based","10.32","Very High","","","De-rusting and painting of main Funnel stack carried out. ","2022-11-15T23:59:35","","Completed","2022-10-10T23:59:35","No","No","No","Internal"]
[null,null,null,27421,59569,"50_Sun Oct 02 2022 23:25:14 GMT+0800","2022-09-15T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Harbour SW pump space heater found not working","Documentation,E/R - Pumps","Eng. / Strg. Comp.","Knowledge Based,Equipment Related","10.32","Very High","","","Harbour SW pump space heater  wire found shorting same rectified and fuse renewed, now working satisfactory.","2022-10-10T23:59:35","","Completed","2022-10-01T23:59:35","No","No","No","Internal"]
[null,null,null,27422,89996,"0_Sun Oct 02 2022 23:37:42 GMT+0800","2022-09-15T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Port Hose Handling Crane operating lever cover found jammed. Cover is to be eased up and made working","Cargo Mach.","Cargo / Ballast Systems","Behaviour Based","8.50","Medium","","","Port Hose Handling Crane operating lever cover freed and eased up for working.","2022-10-10T23:59:35","","Completed","2022-09-28T23:59:35","No","No","No","Internal"]
[null,null,null,27429,18296,"0_Sun Oct 02 2022 23:34:06 GMT+0800","2022-09-15T23:59:35","Non Conformity","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Superintendents’ safety familiarization was not carried out upon joining the vessel within 24 hrs. ","Documentation","Cert. & Docu.","Human Error","5.21","Medium","","","Superintendents’ safety familiarization was carried out upon joining the vessel, at first available opportunity due to vessel's Singapore transit.","2022-09-09T23:59:35","","Completed","2022-09-12T23:59:35","No","No","No","Internal"]
[null,null,null,27430,80781,"0_Sun Oct 02 2022 23:35:45 GMT+0800","2022-09-15T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Life rafts cradle on both Port and Starboard side found rusted. Needs immediate attention","LSA / FFA","Safety / LSA / FFA","Behaviour Based","5.28","Very High","","","Life rafts cradle on both Port and Starboard side de-rusted and painted.","2022-09-22T23:59:35","","Completed","2022-09-18T23:59:35","No","No","No","Internal"]
[null,null,null,27433,47802,"0_Sun Oct 02 2022 23:40:03 GMT+0800","2022-09-15T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Vessels name found not mentioned on few Life vests / jackets. Please checks all Life jackets onboard and ensure vessel name is stenciled in BOLD","LSA / FFA","Safety / LSA / FFA","Knowledge Based","5.32","High","","","All Life jackets/vests onboard checked for proper identification marking. Vests in use are marked with vessel's name in BOLD.","2022-09-22T23:59:35","","Completed","2022-09-20T23:59:35","No","No","No","Internal"]
[null,null,null,27435,75732,"50_Mon Oct 03 2022 01:17:17 GMT+0800","2022-09-15T23:59:35","Non Conformity","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Folder Management System found to updated. Most folders are blank, Deck and Engineer Officers not aware of FMS and FMS not found on vessels PC. ","Documentation","Cert. & Docu.","Knowledge Based","2.3","High","","","Folder management system has been implemented and all engineers and officers has been explained briefed about the system.","2022-10-10T23:59:35","","Completed","2022-09-25T23:59:35","No","No","No","Internal"]
[null,null,null,27436,17067,"0_Sun Oct 02 2022 23:47:47 GMT+0800","2022-09-15T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Proper operating instructions to be posted (stenciled on the bulkhead) for both High and Low Expansion foam systems. ","LSA / FFA","Safety / LSA / FFA","Knowledge Based","5.35","Medium","","","operating poster with photographic illustration posted","2022-10-15T23:59:35","","Completed","2022-09-24T23:59:35","No","No","No","Internal"]
[null,null,null,27437,88698,"0_Mon Oct 03 2022 01:05:15 GMT+0800","2022-09-15T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Forward Emergency Towing booklet still marked for BW Peony and BW Fleet Management Pte Ltd. Vessel and company name to be changed and ETA booklet to be reviewed. ","Documentation","Cert. & Docu.","Behaviour Based","5.13","High","","","Booklet changed with the GSM name .","2022-10-10T23:59:35","","Completed","2022-09-20T23:59:35","No","No","No","Internal"]
[null,null,null,27440,72893,"0_Mon Oct 03 2022 01:18:51 GMT+0800","2022-09-15T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Fixed grinder in the ER workshop found not as per company’s instruction. Grinder should be able to start only when the Emergency stop is pressed. Once the leg is removed from the pedestal, the grinder should STOP. Circuit to be changed accordingly","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Inappropriate Procedure","2.3","High","","","Grinder circuit modification has been carried out as per company instruction ","2022-10-15T23:59:35","","Completed","2022-09-17T23:59:35","No","No","No","Internal"]
[null,null,null,27640,63322,"50_Tue Oct 25 2022 05:32:48 GMT+0800","2022-09-15T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Some of the garbage containers covers were found corroded.","Miscellaneous","MARPOL Related","Behaviour Based","6.20","Medium","","","Garbage container covers were derusted.  Wasted covers were fabricated and replaced. ","2022-10-25T23:59:35","","Completed","2022-10-20T23:59:35","No","No","No","Internal"]
[null,null,null,28718,62288,"50_Tue Jan 31 2023 11:56:39 GMT+0800","2022-09-16T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Fireman walkie talkies battery locking pin broken. Battery becomes loose causing walkies talkie to switch off","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.43","High","","","New Walkie Talkies received. All Faulty walkie talkies replaced ","2023-07-12T23:59:35","DPEO230049","Completed","2023-06-29T23:59:35","No","No","No","Internal"]
[null,null,null,24523,null,"50_22/03/2022 18:49:43","2022-09-16T23:59:35","Observation","Ship Staff","Suptd. Insp.","Fwd hydraulic pump No.1 Pump pressure gauge defective","Deck - Mooring Machinery","Mooring","Equipment Related","9.14","Medium","","","Replaced with new pressure gauge. Requisiton raised for one spare.\n\n\t\n\t\n","2023-01-26T23:59:35","","Completed","2023-02-09T23:59:35","No","No","No","Internal"]
[null,null,null,24544,null,"50_23/03/2022 18:21:23","2022-09-16T23:59:35","Observation","Ship Staff","Suptd. Insp.","Check M/eng F.O Viscosity controller.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","M/E F.O. VISCOSITY CONTROLLER, checked the connection of power supply and fuse and found working satisfactory.","2023-10-03T23:59:35","DPEO 230230 - Cancelled","Completed","2023-10-10T23:59:35","No","No","No","Internal"]
[null,null,null,24545,null,"50_23/03/2022 18:26:03","2022-09-16T23:59:35","Observation","Ship Staff","Suptd. Insp.","Check D/G  F.O Viscosity controller.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","AE #1&2 F.O. VISCOSITY CONTROLLER checked and corrected the power supply connection and indication stated showing.","2023-10-03T23:59:35","DPEO 230230","Completed","2023-10-10T23:59:35","No","No","No","Internal"]
[null,null,null,27402,94080,"50_Sun Oct 02 2022 21:40:42 GMT+0800","2022-09-25T23:59:35","Observation","Ship Staff","Ship Staff Insp.","IG scrubber tower overboard line got soft patches","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","SECTION OF WASTED PIPELINES(4 IN NOS) RENEWED WITH NEW ONE, TRIED OUT FOUND WORKING SATISFACTORY, NO LEAKS","2022-12-25T23:59:35","","Completed","2023-01-05T23:59:35","No","No","No","Internal"]
[null,null,null,27403,42687,"50_Sun Oct 02 2022 21:50:33 GMT+0800","2022-09-25T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Fire & GS pp 1 outlet pipe  have  soft patch","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.31","Very High","","","fire & GS pp # 1 outlet pipe removed and permanent repair carried out, fitted back and tried out found satisfactory","2022-11-10T23:59:35","","Completed","2022-10-06T23:59:35","No","No","No","Internal"]
[null,null,null,27634,13436,"50_Mon Oct 03 2022 13:17:23 GMT+0800","2022-09-26T23:59:35","Defect","Ship Staff","Ship Staff Insp.","A.E.3 Turbo charger RPM sensor defective","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Renewed from spare.","2023-04-25T23:59:35","DPEO220166","Completed","2023-04-22T23:59:35","No","No","No","Internal"]
[null,null,null,27417,89217,"50_Mon Oct 03 2022 10:58:17 GMT+0800","2022-09-27T23:59:35","Defect","Ship Staff","Ship Staff Insp.","ODM Sea Chest sampling line holed in pumproom.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.8","Medium","","","ODM Sea Chest sampling line fabricated and refitted.","2022-10-25T23:59:35","","Completed","2022-10-13T23:59:35","No","No","No","Internal"]
[null,null,null,27418,53001,"0_Mon Oct 03 2022 11:00:52 GMT+0800","2022-09-27T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Deck seal overflow pipe found leaking in pumproom.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.30","High","","","Deck seal overflow pipe fabricated and placed back in position.  deck seal pump started and pipe integrity tested.","2022-10-25T23:59:35","","Completed","2022-10-11T23:59:35","No","No","No","Internal"]
[null,null,null,27632,24971,"50_Sat Oct 29 2022 09:39:44 GMT+0800","2022-09-30T23:59:35","Defect","Ship Staff","Ship Staff Insp."," pipe to suction manifold for fire, bilge & GS pump # 2 holed","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Corroded pipe section renewed with insert, job exported to REFMAN with office advice need to renew all pipe in DD","2022-11-25T23:59:35","","Completed","2022-11-16T23:59:35","No","No","No","Internal"]
[null,null,null,27637,47431,"50_Sat Oct 08 2022 08:57:17 GMT+0800","2022-10-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","AE#3  JACKET PREHEATER HEATER GAVE 440V LOW INSULATION ALARM.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","SYSTEM ISOLATED, AND INSPECTION CARRIED OUT, FOUND GROUNDING WIRE CONNECTON WITH PHASE, SAME ISOLATED AND SECURED .","2022-10-02T23:59:35","","Completed","2022-10-01T23:59:35","No","No","No","Internal"]
[null,null,null,27639,42728,"50_Mon Oct 10 2022 14:48:42 GMT+0800","2022-10-01T23:59:35","Observation","Ship Staff","Ship Staff Insp.","EGCS SW PP # 1 SUCTION PIPE GOT HOLED SAME TEMPORARY REPAIR CARRIED OUT NEED TO RENEW","","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","EGCS SW PP # 1  SUCTION PIPE DAMAGED PIPE SECTION RENEWED WITH NEW PIPE FABRICATION , PIPE FITTED BACK AND TRIED  OUT FOUND SATISFACTORY.","2022-10-09T23:59:35","","Completed","2022-10-05T23:59:35","No","No","No","Internal"]
[null,null,null,27644,46247,"50_Tue Oct 18 2022 14:25:19 GMT+0800","2022-10-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","During derusting of stbd side manifold pipelines, marpol line sampling pipe found holed.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.41","Medium","","","Fabrication of Sampling pipe of marpol line carried out and refitted.","2022-10-25T23:59:35","","Completed","2022-10-13T23:59:35","No","No","No","Internal"]
[null,null,null,24548,null,"50_23/03/2022 18:32:25","2022-10-02T23:59:35","Observation","Ship Staff","Suptd. Insp.","IG Scrubber NR FLAP VALVE to replace","Inert Gas","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Renewed at singapore.","2023-01-26T23:59:35","","Completed","2023-03-18T23:59:35","No","No","No","Internal"]
[null,null,null,27642,70784,"50_Tue Nov 01 2022 11:11:49 GMT+0800","2022-10-02T23:59:35","Defect","Ship Staff","Ship Staff Insp.","During derusting of stbd manifold pipelines, bunker drain line to 3 stbd cot found holed.","Deck - Pipe / Fittings","MARPOL Related","Equipment Related","8.41","Medium","","","fabrication of the bunker drain line carried out and wasted pipe replaced with fabricated line.","2022-10-26T23:59:35","","Completed","2022-10-26T23:59:35","No","No","No","Internal"]
[null,null,null,27638,49662,"50_Mon Oct 10 2022 17:20:16 GMT+0800","2022-10-03T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Two cooking range found Not working.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","11.13","Low","","","Ship staff investigated and repaired one cooking range and renewed one. Now all are in good working condition.","2022-10-10T23:59:35","","Completed","2022-10-05T23:59:35","No","No","No","Internal"]
[null,null,null,27645,79219,"50_Wed Oct 12 2022 15:24:35 GMT+0800","2022-10-06T23:59:35","Observation","Ship Staff","Ship Staff Insp.","EGCS SW  pp# 2 discharge pipe leaking ","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","pipe section removed from place and corroded secion cropped and renewed .","2022-11-25T23:59:35","","Completed","2022-11-11T23:59:35","No","No","No","Internal"]
[null,null,null,27643,68950,"50_Wed Oct 12 2022 15:19:53 GMT+0800","2022-10-07T23:59:35","Observation","Ship Staff","Ship Staff Insp.","ME Jacket cooling water buffer tank gauge not functional","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Gaug glass opened up and overhualed and made operational","2022-11-07T23:59:35","","Completed","2022-11-06T23:59:35","No","No","No","Internal"]
[null,null,null,27641,57071,"50_Mon Oct 31 2022 04:12:28 GMT+0800","2022-10-10T23:59:35","Observation","Ship Staff","Ship Staff Insp.","EMERGENCY FIRE PUMP WHEN STARTED GIVING 440V LOW INSULATION.","Critical Equip.","Emgcy. Systems","External Factors","5.35","Medium","","","INSPECTION CARRIED OUT, FOUND TERMINAL ENTERANCE CABLE GIVING ISSUE, SAME ROMOVED INSPECTED CLEANED CABLES INSIDE TERMINAL BOX INSULATED . AND TESTED AFTER CONNECTION, WORKING SATISFACTORY.","2022-10-15T23:59:35","","Completed","2022-10-13T23:59:35","No","No","No","Internal"]
[null,null,null,27631,34640,"50_Sat Oct 29 2022 09:36:37 GMT+0800","2022-10-13T23:59:35","Defect","Ship Staff","Ship Staff Insp.","FIRE & GS PP # 1 suction pipe pin hole","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Fire & GS pp # 1 suction pipe renewed with new fabricated pipe section","2022-11-25T23:59:35","","Completed","2022-11-16T23:59:35","No","No","No","Internal"]
[null,null,null,27646,95175,"50_Sat Oct 29 2022 09:32:30 GMT+0800","2022-10-13T23:59:35","Defect","Ship Staff","Ship Staff Insp.","EGCS SW pump # 2 outlet pipe pin hole in the welding seam","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","pipe section removed and corroded section pipe cropped and renewed  and fixed back","2022-11-25T23:59:35","","Completed","2022-11-11T23:59:35","No","No","No","Internal"]
[null,null,null,24521,null,"50_22/03/2022 18:02:00","2022-10-16T23:59:35","Observation","Ship Staff","Suptd. Insp.","COW line soft patch to repair","Cargo Mach.,Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","11.4","Very High","","","COW LINE PENETRATING FROM PUMP ROOM TO DECK HAS SOFT PATCH. NEED TO PLAN FOR PERMANENT SOLUTION.\nSHIP’S STAFF COMMENTS: CARGO TANK NEED TO BE GAS FREE OR JOB TO BE SHIFTED TO NEXT DRY DOCK, KINDLY ADVISED.\nJob updated in Refman","2023-06-26T23:59:35","","Completed","2023-06-09T23:59:35","No","No","No","Internal","Job shifted to Refman."]
[null,null,null,24522,null,"50_22/03/2022 18:35:26","2022-10-16T23:59:35","Observation","Ship Staff","Suptd. Insp.","Spring line mooring winch has delay of 10 to 15 sec while starting ,abanormal noise when started .","Deck - Mooring Machinery","Mooring","Equipment Related","9.7","Medium","","","SHIP’S STAFF COMMENTS: UNIT HAS BEEN PURGED AND TESTED. OPERATION SPEED FOUND TO BE NORMAL . NOISE COMES FROM THE SYSTEM WHEN OPERATED SUDDENLY , WHEN OPERATED GRADUALLY OPERATION FOUND TO BE IN ORDER.\nJOB CLOSED OUT AS PER OFFICE ADVICE.,","2022-12-26T23:59:35","","Completed","2022-12-01T23:59:35","No","No","No","Internal","PLEASE PURGE THE UNIT AND TEST AGAIN.,\nCLOSE THE JOB "]
[null,null,null,27633,33710,"50_Mon Oct 31 2022 04:25:52 GMT+0800","2022-10-18T23:59:35","Observation","Ship Staff","Ship Staff Insp.","220V insulation meter in MSB needle sometimes get stuck, 440V and 220V galley and forward insulation meters  needle donot move while testing with earth switch.","Elect. Mach. & Equip.","General Appearance","Equipment Related","5.43","High","","","CHECKED FOUND WORKING SATISFACTORILY.","2023-05-25T23:59:35","DPEO220285","Completed","2023-04-29T23:59:35","No","No","No","Internal"]
[null,null,null,27635,81979,"50_Sat Nov 19 2022 00:56:13 GMT+0800","2022-10-24T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","MAIN FIRE ALARM PANEL ON BRIDGE SHOWING REPEATER NOT INSTALLED ON THE PANEL AND REPEATER ON THE ECR IS NOT SHOWING ANY VALUE ON THE SCREEN.","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.35","Medium","","","vessel received the spare repeater and fixed in place now working satisfactory.","2022-12-25T23:59:35","PO NO. DPEO 220289 - FIRE ALARM REPEATER PANEL","Completed","2022-12-06T23:59:35","No","No","No","Internal"]
[null,null,null,28717,63816,"50_Tue Jan 31 2023 11:53:31 GMT+0800","2022-10-27T23:59:35","Observation","Ship Staff","Ship Staff Insp.","No.5 fire line isolation valve very hard to operate","Accommodation,LSA / FFA","Safety / LSA / FFA","Human Error","5.38","High","","","REPLACED WITH NEW ISLO VALVE WHICH RECIEVED IN SINGAPORE","2023-03-25T23:59:35","DPEO230047","Completed","2023-03-30T23:59:35","No","No","No","Internal"]
[null,null,null,27807,84845,"50_Sun Nov 27 2022 06:35:30 GMT+0800","2022-10-28T23:59:35","Defect","Ship Staff","Ship Staff Insp.","During derusting port side manifold marpol line sampling line found wasted.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.41","Medium","","","Fabrication of wasted marpol line sampling line carried out.","2022-11-25T23:59:35","","Completed","2022-11-19T23:59:35","No","No","No","Internal"]
[null,null,null,27414,74737,"0_Mon Oct 03 2022 00:52:50 GMT+0800","2022-10-31T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Main Engine Starting Air Inlet Pressure gauge in the ECR console found not working","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Spare module fitted for the transmitter found working satisfactorily.","2023-05-26T23:59:35","DPEO230026","Completed","2023-05-09T23:59:35","No","No","No","Internal"]
[null,null,null,27636,79113,"50_Sat Nov 19 2022 01:11:33 GMT+0800","2022-10-31T23:59:35","Defect","Ship Staff","Ship Staff Insp.","8 in nos the electric horns of the signal coloumn light not working.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.35","Very High","","","Renewed from spare. Working satisfactorily.","2023-04-25T23:59:35","PO NO. DPEO - 220294\n              DPEO - 220180","Completed","2023-04-01T23:59:35","No","No","No","Internal"]
[null,null,null,27400,68499,"50_Sun Oct 02 2022 20:27:59 GMT+0800","2022-11-05T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Ship Staff Insp.","U clamps of pipelines on main deck corroded","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.5","Medium","","","Derusting and painting of deck pipe lines completed.\nRoutinue maintenance is in progress at all times","2023-05-26T23:59:35","","Completed","2023-05-21T23:59:35","No","No","No","Internal"]
[null,null,null,27963,62502,"50_Tue Dec 13 2022 23:47:35 GMT+0800","2022-11-05T23:59:35","Defect","Ship Staff","Ship Staff Insp.","SALINITY AND TEMP SENSOR OF BWTS NOT WORKING ","Miscellaneous","MARPOL Related","Equipment Related","4.6","Medium","","","Renewed from spare and tried out working satisfactorily.","2023-03-26T23:59:35","DPEO220324- BWTS SPARES (SALINITY SENSOR AND EOCR)","Completed","2023-03-26T23:59:35","No","No","No","Internal"]
[null,null,null,27964,49186,"50_Tue Dec 13 2022 23:52:31 GMT+0800","2022-11-06T23:59:35","Defect","Ship Staff","Ship Staff Insp.","BWTS PUMP ROOM FILTER #2 MOTOR EOCR SHOWING ERROR.","Cargo Mach.","MARPOL Related","Equipment Related","4.20","Very High","","","ISSUE  RESOLVED","2023-08-26T23:59:35","DPEO220324- BWTS SPARES (SALINITY SENSOR AND EOCR)","Completed","2023-07-19T23:59:35","No","No","No","Internal"]
[null,null,null,27808,52768,"50_Tue Dec 06 2022 09:56:21 GMT+0800","2022-11-18T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Port gangway gear oil box sight glass found broken.","Deck - Machinery","Safety / LSA / FFA","Behaviour Based","5.47","Medium","","","port gangway sight glass repaired and fitted back","2022-12-25T23:59:35","","Completed","2022-11-19T23:59:35","No","No","No","Internal"]
[null,null,null,29489,60528,"50_Wed Mar 08 2023 11:27:10 GMT+0800","2022-11-23T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Departure Rizhou; Entry for switching BNWAS “ON” missing ","Navigation - Others","Navigation","Human Error","","","","","Log book checked for missing entries\nEntry for switching \"ON\" BNWAS made in log book.","2023-02-22T23:59:35","","Completed","2022-11-23T23:59:35","No","No","No","Internal"]
[null,null,null,29490,69393,"50_Wed Mar 08 2023 11:31:26 GMT+0800","2022-11-23T23:59:35","Non Conformity","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Arrival Singapore entry for completion of Pre arrival checklist 12.01.34.081.03 indicates entire Checklist has been completed instead of only Section 1 of the checklist.","Navigation - Others","Navigation","Human Error","","","","","All OOW briefed on importance of log book entries and instructed to  update same religiously","2023-02-22T23:59:35","","Completed","2022-11-23T23:59:35","No","No","No","Internal"]
[null,null,null,29491,21764,"50_Wed Mar 08 2023 11:35:30 GMT+0800","2022-11-23T23:59:35","Non Conformity","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Form 12.01.10.021.00 used for Passage plan not from QDMS","Navigation - Others","Navigation","Human Error","","","","","12.01.10.021.00 Passage plan checklist downloaded from QDMS and filled.All OOW briefed on importance of using updated checklist from QDMS to avoid any remarks in future.","2023-02-22T23:59:35","","Completed","2022-11-25T23:59:35","No","No","No","Internal"]
[null,null,null,27962,16956,"50_Tue Dec 13 2022 23:33:34 GMT+0800","2022-11-30T23:59:35","Defect","Ship Staff","Ship Staff Insp.","EGCS NO #3 SEAWATER PUMP TRIPPING ON DRIVE OVER HEAT ALARM AND NOT BUILDING UP PRESSURE.","E/R - Pumps","MARPOL Related","Equipment Related","5.19","Medium","","","HEAT SINK FAN RENEWED , PUMP OVERHAULED AND FOUND THE CASING GASKET SIZE OF 2.5MM (SHOULD HAVE BEEN FACE TO FACE OR PAPER GASKET) BEING INSTALLED IN THE PUMP DURING PREVIOUS OVERHAUL AND THE THE IMPELLER O RING DAMAGED. RECTIFIED THE SAME.TRIED OUT. PRESENTLY BUILDING UP PRESSURE AND RUNNING AT RATED AMPERES OF 100A AT 85% LOAD.","2023-02-10T23:59:35","","Completed","2023-01-19T23:59:35","No","No","No","Internal"]
[null,null,null,28712,87755,"50_Tue Jan 31 2023 12:01:18 GMT+0800","2022-12-01T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Lifeboat first aid kit expiring in Jan 2023","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.29","High","","","REQUISITION RECIVED AT SINGAPORE ON 21 MAR 2023.\nREPLACED WITH NEW ITEM","2023-03-25T23:59:35","DPEO230001","Completed","2023-03-19T23:59:35","No","No","No","Internal"]
[null,null,null,27960,93079,"50_Mon Dec 12 2022 02:21:28 GMT+0800","2022-12-06T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Fwd L.T. cooler Pin hole leak from overboard discharge line","E/R - Pipes/ valves & fittings","","Equipment Related","10.32","Very High","","","LEAKING PIPE SECTION RENEWED WITH NEW FABRICATED PIPE SCETION.","2023-01-26T23:59:35","","Completed","2023-02-25T23:59:35","No","No","No","Internal"]
[null,null,null,27961,64002,"50_Tue Dec 13 2022 13:30:17 GMT+0800","2022-12-06T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Grey water direct overboard valve leaking , sewage direct overboard valve stuck in closed position.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Valve renewed at Singapore during underhull cleaning.","2023-01-26T23:59:35","DPEO220304","Completed","2023-03-18T23:59:35","No","No","No","Internal"]
[null,null,null,27965,86157,"50_Wed Dec 21 2022 06:27:10 GMT+0800","2022-12-14T23:59:35","Observation","Ship Staff","Ship Staff Insp.","REEFER Compressor no.1  making noise while running .","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Compressor dismantled and found piston clearance  high on pin area  , same replaced from  spare compressor , tried out the compressor found satisfactory","2022-12-26T23:59:35","","Completed","2022-12-19T23:59:35","No","No","No","Internal"]
[null,null,null,28171,45928,"0_Tue Dec 27 2022 05:27:29 GMT+0800","2022-12-15T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Drop valve CAV 164 indicator lamp not working","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.11","Medium","","","DDRL  already included in another item.","2023-03-14T23:59:35","","Completed","2023-02-15T23:59:35","No","No","No","Internal"]
[null,null,null,28172,72754,"0_Tue Dec 27 2022 05:32:10 GMT+0800","2022-12-15T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Two Self Igniting light found expired.","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.31","High","","","REQUISITION RECIVED AT SINGAPORE ON 21 MAR 2023.\nREPLACED WITH NEW ITEM","2023-03-14T23:59:35","DPEO230001","Completed","2023-03-19T23:59:35","No","No","No","Internal"]
[null,null,null,28173,10143,"50_Tue Dec 27 2022 05:29:48 GMT+0800","2022-12-15T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Various pressure gauges in CCR non-operational. No.1 cargo eductor drive gauge, No.1 cargo eductor suction gauge, No.2 cargo eductor drive gauge, No.1 COP suction px gauge, No.3 COP suction px gauge, No.1 manifold pressure gauge","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.15","High","","","Repairs and calibration carried out.","2023-03-14T23:59:35","","Completed","2023-01-27T23:59:35","No","No","No","Internal"]
[null,null,null,28174,47949,"50_Tue Dec 27 2022 05:26:11 GMT+0800","2022-12-15T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Water ballast tank 2P main valve operating issue from CCR panel.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.11","Medium","","","Valve is operating from CCR.","2023-03-14T23:59:35","","Completed","2023-02-15T23:59:35","No","No","No","Internal"]
[null,null,null,28175,14959,"0_Tue Dec 27 2022 05:39:28 GMT+0800","2022-12-15T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","•\tSafety posters for ER (Gas cutting /welding) missing","Miscellaneous,LSA / FFA","Safety / LSA / FFA","Knowledge Based","5.25","Medium","","","REQUISITION RECIVED AT SINGAPORE ON 21 MAR 2023.\nSAFETY POSTER POSTED IN WORKSHOP","2023-03-19T23:59:35","DPEO230093","Completed","2023-03-19T23:59:35","No","No","No","Internal"]
[null,null,null,28176,94424,"0_Tue Dec 27 2022 06:32:28 GMT+0800","2022-12-15T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","VECS reducers missing the guide studs ","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.17","Low","","","Reducers fitted with missing guides.","2023-03-14T23:59:35","","Completed","2023-01-26T23:59:35","No","No","No","Internal"]
[null,null,null,28177,89770,"0_Tue Dec 27 2022 05:44:07 GMT+0800","2022-12-15T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Steering gear room stbd bilge suction access obstructed with drums and items stored","Miscellaneous","Eng. / Strg. Comp.","Knowledge Based","10.42","Medium","","","All drums  removed and space cleared, bilge area marked","2023-03-14T23:59:35","","Completed","2022-12-30T23:59:35","No","No","No","Internal"]
[null,null,null,28178,53033,"0_Tue Dec 27 2022 05:47:55 GMT+0800","2022-12-15T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Lifeboat hatch packing not sealing ","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.29","High","","","Lifeboat hatch rubber packing doubled up. Locking wedges build up for proper securing.  ","2023-03-14T23:59:35","DPEO230050","Completed","2023-01-08T23:59:35","No","No","No","Internal"]
[null,null,null,28179,87477,"0_Tue Dec 27 2022 06:00:12 GMT+0800","2022-12-15T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Calcification noted on bridge wing sockets for VHF and Aldis lamp","Navigation - Others","General Appearance","Behaviour Based","11.16","Low","","","Bridge wing sockets for VHF and Aldis lamp cleared of calcification and covered to prevent from such conditions.","2023-03-14T23:59:35","","Completed","2022-12-20T23:59:35","No","No","No","Internal"]
[null,null,null,28180,10257,"0_Tue Dec 27 2022 06:30:54 GMT+0800","2022-12-15T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Unloader for VRCS not operational, VRCS system unable to maintain Hydraulic pressure during operations","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.11","Medium","","","New unloader received and replaced, VRCS system now maintaining required pressure with pump cut in cut off happening normally","2023-07-26T23:59:35","DPEO230134","Completed","2023-07-01T23:59:35","No","No","No","Internal"]
[null,null,null,28181,70381,"0_Tue Dec 27 2022 06:34:32 GMT+0800","2022-12-15T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Numerous drums secured on Funnel decks – discard eroded drums","Accommodation","General Appearance","Behaviour Based","11.8","Low","","","Drums offlanded at Singapore","2023-03-14T23:59:35","","Completed","2023-03-17T23:59:35","No","No","No","Internal"]
[null,null,null,28182,88485,"0_Wed Dec 28 2022 01:58:28 GMT+0800","2022-12-15T23:59:35","Non Conformity","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Latest copies of the CBA to be made available to the crew (MLC files located in the recreation rooms) including \n-Copies of the Manning office license (RPSL) and Audit reports not available on board.\n-Annex to MUI CBA referring to the Wages for Additional Officers and Cadets\n-AMOUSUP/ ITF-TCCC Non IBF and Indonesian CBA referring to the RT OS\n","Documentation","MLC Related","Behaviour Based","","","","","All the latest files of CBA made available to all crew as per their nationalities.","2023-03-14T23:59:35","","Completed","2023-01-20T23:59:35","No","No","No","Internal"]
[null,null,null,28183,43572,"0_Wed Dec 28 2022 02:30:00 GMT+0800","2022-12-15T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Steam Coils for Slop P not pressure tested since DD in 2021","Cargo Mach.","Cargo / Ballast Systems","Behaviour Based","8.15","High","","","Pressure testing of steam coils carried out.","2023-03-14T23:59:35","","Completed","2023-01-20T23:59:35","No","No","No","Internal"]
[null,null,null,28184,92477,"0_Wed Dec 28 2022 02:32:35 GMT+0800","2022-12-15T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Annual Pressure test for Cargo lines carried out to 12.5 kg/cm2 while MWAP of the pipelines is 15.7 Kg/cm2","Deck - Pipe / Fittings","Cargo / Ballast Systems","Knowledge Based","8.13","Medium","","","Pressure testing of cargo lines carried out upto 15.7 Kg/cm2.","2023-03-14T23:59:35","","Completed","2023-01-19T23:59:35","No","No","No","Internal"]
[null,null,null,28186,60934,"0_Wed Dec 28 2022 02:18:25 GMT+0800","2022-12-15T23:59:35","Non Conformity","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Pictorial procedure for Use of IG to Ballast Tanks not ship specific","Cargo Mach.","Cargo / Ballast Systems","Behaviour Based","","","","","New ship specific emergency IG inerting of ballast tanks pictorial procedure prepared and posted.","2023-03-14T23:59:35","","Completed","2023-01-23T23:59:35","No","No","No","Internal"]
[null,null,null,28187,46110,"50_Wed Dec 28 2022 02:27:05 GMT+0800","2022-12-15T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Mushroom vents on Poop deck and fwd frozen, To be lubricated","Deck - Machinery","Safety / LSA / FFA","Behaviour Based","","","","","Mushroom vent on the poop deck opened overhauled, repairs carried out. ","2023-03-14T23:59:35","","Completed","2022-12-29T23:59:35","No","No","No","Internal"]
[null,null,null,28189,46947,"50_Wed Dec 28 2022 01:46:28 GMT+0800","2022-12-15T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Pipelines stored in the athwartship direction without end plates","Deck - Pipe / Fittings","General Appearance","Knowledge Based","4.4","High","","","vessel will shift the concerned pipes to respective location.","2023-07-26T23:59:35","","Completed","2023-07-10T23:59:35","No","No","No","Internal"]
[null,null,null,28190,57613,"0_Wed Dec 28 2022 02:20:40 GMT+0800","2022-12-15T23:59:35","Non Conformity","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Hyper mist system FW Tank feed valves not marked, sealed in open condition with poster / warning to prevent accidental closure.","LSA / FFA","Safety / LSA / FFA","Behaviour Based","","","","","Hyper mist tank minimum level to be maintain marked and suction valve from tank locked open postion and poster posted.","2023-03-14T23:59:35","","Completed","2022-12-31T23:59:35","No","No","No","Internal"]
[null,null,null,28191,36562,"0_Wed Dec 28 2022 02:19:12 GMT+0800","2022-12-15T23:59:35","Non Conformity","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Waste Oil drum in Gally not fire retardant, not colour coder, not lashed","LSA / FFA","Safety / LSA / FFA","Behaviour Based","","","","","Galley waste oil drum changed to metal drum,  fire retartant with company specific colour coding and lashing.","2023-03-14T23:59:35","","Completed","2022-12-16T23:59:35","No","No","No","Internal"]
[null,null,null,28192,96005,"0_Wed Dec 28 2022 01:48:37 GMT+0800","2022-12-15T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Stbd Accommodation ladder motor unable to swing out ladder","Deck - Machinery","Safety / LSA / FFA","Equipment Related","5.47","Medium","","","Pneumatic motor overhauled and veins renewed. ","2023-03-14T23:59:35","","Completed","2022-12-17T23:59:35","No","No","No","Internal"]
[null,null,null,28193,52247,"0_Wed Dec 28 2022 02:22:20 GMT+0800","2022-12-15T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Lifeboat launching procedure posted at Lifeboat stations not ship specific- applicable to vessel’s launching arrangements","LSA / FFA","Safety / LSA / FFA","Knowledge Based","5.27","Medium","","","Ship specific Lifeboat launching procedure posted at Lifeboat stations - applicable to vessel’s launching arrangements","2023-03-14T23:59:35","","Completed","2022-12-16T23:59:35","No","No","No","Internal"]
[null,null,null,28194,63080,"0_Tue Dec 27 2022 05:54:35 GMT+0800","2022-12-15T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Burning vessel symbol for Fire plan location not in line with requirements","LSA / FFA","Safety / LSA / FFA","Behaviour Based","5.37","Low","","","Burning vessel symbol for Fire plan posted as per requirements","2023-03-14T23:59:35","","Completed","2022-12-18T23:59:35","No","No","No","Internal"]
[null,null,null,28195,19876,"0_Wed Dec 28 2022 02:01:02 GMT+0800","2022-12-15T23:59:35","Non Conformity","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Pre-joining Medical examination report for the Trainee Electrical Officer not available on board","Documentation","MLC Related","Behaviour Based","","","","","Received Medical report From FPD","2023-03-14T23:59:35","","Completed",null,"No","No","No","Internal"]
[null,null,null,28196,14920,"0_Wed Dec 28 2022 01:52:45 GMT+0800","2022-12-15T23:59:35","Non Conformity","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Procedures upon receipt of Distress messages (Company standing orders and SOLAS chap V Reg 33) not complied with","Navigation - GMDSS & Communication","Communication","Behaviour Based","4.21","High","","","All OOW  were explained regarding Procedures upon receipt of Distress messages (Company standing orders and SOLAS chap V Reg 33) by master ,And correct entry made GMDSS log ","2023-03-14T23:59:35","","Completed",null,"No","No","No","Internal"]
[null,null,null,28197,68149,"0_Tue Dec 27 2022 05:53:18 GMT+0800","2022-12-15T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Launching Lifeboats in dangerous atmosphere procedure faded","LSA / FFA","Safety / LSA / FFA","Behaviour Based","5.29","High","","","Launching Lifeboats in dangerous atmosphere procedure renewed.","2023-03-14T23:59:35","","Completed","2022-12-16T23:59:35","No","No","No","Internal"]
[null,null,null,28198,57791,"0_Tue Dec 27 2022 05:34:59 GMT+0800","2022-12-15T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Fire hydrant caps not having pressure relief holes/ painted over","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.35","Medium","","","Some of the Fire hydrant caps pressure relief holes found painted - paint removed.\nSome of the fire hydrant caps doe snot have pressure relief holes - holes fabricated for pressure relief. ","2023-03-14T23:59:35","","Completed","2022-12-16T23:59:35","No","No","No","Internal"]
[null,null,null,29483,83958,"50_Tue Feb 14 2023 10:53:29 GMT+0800","2022-12-18T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","•\tStbd Accommodation ladder motor unable to swing out ladder","Deck - Machinery","ISM Related","Equipment Related","","","","","Motor overhauled and repairs carried out.","2023-02-23T23:59:35","","Completed","2023-02-10T23:59:35","No","No","No","Internal"]
[null,null,null,28185,66389,"50_Sat Dec 31 2022 06:16:32 GMT+0800","2022-12-19T23:59:35","Observation","Ship Staff","Ship Staff Insp.","2 Port Buker tank remote level guage not working","Hull & Tanks","Eng. / Strg. Comp.","Equipment Related","","","","","sensor renewed. at next opertunity, open the tank and clean the internal air pipe. ","2023-07-26T23:59:35","DPEO230201","Completed","2023-07-16T23:59:35","No","No","No","Internal"]
[null,null,null,29484,32841,"50_Wed Mar 08 2023 10:27:27 GMT+0800","2022-12-24T23:59:35","Critical Equipment","Ship Staff","Nav Audit / Verification","Manual hand pull whistle wire found jammed for main mast whistle. Unable to operate manually from wheelhouse.","Navigation - Others","Navigation","Equipment Related","","","","","Whistle wire/pulley made free from paint to operate whistle manually from wheel house.","2023-03-24T23:59:35","","Completed","2023-01-24T23:59:35","No","No","No","Internal"]
[null,null,null,29485,98903,"50_Wed Mar 08 2023 10:31:45 GMT+0800","2022-12-24T23:59:35","Observation","Ship Staff","Nav Audit / Verification","WBT sounding & last port departure data not updated in deck log book.","Navigation - Others","Navigation","Human Error","","","","","All required Entries made in Deck log book.","2023-03-24T23:59:35","","Completed","2023-01-24T23:59:35","No","No","No","Internal"]
[null,null,null,29486,64086,"50_Wed Mar 08 2023 10:35:12 GMT+0800","2022-12-24T23:59:35","Other","Ship Staff","Nav Audit / Verification","No designated bag found for carrying documents during an emergency. Same to be prepared and kept ready.","Miscellaneous","Navigation","Human Error","","","","","Designated bag prepared for Documents in case of emergency.","2023-03-24T23:59:35","","Completed","2023-01-24T23:59:35","No","No","No","Internal"]
[null,null,null,28702,17429,"0_Mon Jan 30 2023 15:10:11 GMT+0800","2022-12-25T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Many COW machines have developed leaks from O-rings/gaskets","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","17 COW machines turbine gear housing o rings and Shaft oil seal replaced. \nAnother 5 COW machines seals and O rings renewed, at present no COW machines are leaking.","2023-06-27T23:59:35","DPEO220252","Completed","2023-06-28T23:59:35","No","No","No","Internal"]
[null,null,null,28703,72449,"50_Mon Jan 30 2023 15:04:30 GMT+0800","2022-12-25T23:59:35","Observation","Ship Staff","Ship Staff Insp.","WBT Remote gauging system defective for various tanks 1S, 5P, 5S, 4S, shows erratic reading for other few tanks","Cargo Mach.","","Equipment Related","8.15","High","","","Level datic system in hydraulic room individual units opened and stuck and rusted springs cleaned. Lines to the ballast tanks blown through.\n16/05/2023\nConstatnt speed controller in level datic system found as root cause of problem, Spring and diaphragm mechanism inside found broken/corroded.  For 1Stbd and 4S overhauled same now working\n5P and 5S required spares ordered\n\n22 May 2023\nWork completed, all Ballast guages working after shore technician visist and servicing of the system","2023-05-25T23:59:35","","Completed","2023-05-18T23:59:35","No","No","No","Internal"]
[null,null,null,28704,10870,"0_Mon Jan 30 2023 15:44:25 GMT+0800","2022-12-25T23:59:35","Observation","Ship Staff","Ship Staff Insp.","SAAB shows \"IO terminal bus1 ground fail\". Does not display any drafts","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.15","High","","","FOUND ONE CONNECTION DISCONNECTED AND TOUCHING GROUND","2023-03-24T23:59:35","","Completed","2023-03-09T23:59:35","No","No","No","Internal"]
[null,null,null,28705,90285,"50_Mon Jan 30 2023 15:13:57 GMT+0800","2022-12-25T23:59:35","Observation","Ship Staff","Ship Staff Insp.","All PV valves are leaking.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.39","Medium","","","PV valves vacuum and pressure side discs renewed with the one received. Leaks on PV valves arrested ","2023-04-25T23:59:35","DPEO220305","Completed","2023-04-25T23:59:35","No","No","No","Internal"]
[null,null,null,28706,21670,"0_Mon Jan 30 2023 15:33:55 GMT+0800","2022-12-25T23:59:35","Observation","Ship Staff","Ship Staff Insp.","BWTS no.2 filter px-tx inlet outlet gauges not working. Differential pressure data unavailable. BWTS No 1 filter BT1213 bypass valve operates on manual mode locally from pumproom using portable handpump, Remote operation from CCR not working. BWTS No2 filter BT2213 bypass valve operates on manual mode locally from pumproom using handpump, remote operation from CCR not working. BWTS v/v BV23 solenoid S/F fail, no auto operation. BWTS sensor for salinity & temperature removed. Local read out (Valve indication) not visible for No.1 filter inlet valve BT 1211. BWTS non-operational during deballasting ops in Brazil","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.15","High","","","new screen replaced and working in good order. ","2023-08-27T23:59:35","","Completed","2023-07-09T23:59:35","No","No","No","Internal"]
[null,null,null,28707,79462,"50_Mon Jan 30 2023 15:41:42 GMT+0800","2022-12-25T23:59:35","Observation","Ship Staff","Ship Staff Insp.","CAV 176, CAV 164 open-shut indicators do not show their status, when in fully open or shut condition","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.15","High","","","VALVE CAV 176 ISSUE SOLVED Defect checked. \nCAV 164 SPARES RECEVD AND RENEWED, ISSUE RESOLVED","2023-07-14T23:59:35","DPEO230045","Completed","2023-07-01T23:59:35","No","No","No","Internal"]
[null,null,null,28711,62444,"0_Mon Jan 30 2023 15:08:00 GMT+0800","2022-12-25T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Midship draft gauges non-operational. Fwd and aft draft gauges not showing any value.","Miscellaneous","Cargo / Ballast Systems","Equipment Related","","","","","Completed by service technicians at singapore","2023-07-26T23:59:35","","Completed","2023-03-17T23:59:35","No","No","No","Internal"]
[null,null,null,28361,70958,"50_Mon Jan 16 2023 03:47:05 GMT+0800","2022-12-27T23:59:35","Observation","Ship Staff","Ship Staff Insp.","MAIN FEED PP # 1 MECHANICAL SEAL LEAK","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Renewed the suction casing and tried out found developing 26bars.","2023-05-26T23:59:35","DPEO230011","Completed","2023-05-17T23:59:35","No","No","No","Internal"]
[null,null,null,28188,14593,"50_Mon Jan 02 2023 22:52:43 GMT+0800","2022-12-28T23:59:35","Defect","Ship Staff","Ship Staff Insp.","BOTH LIFEBOATS (PORT & STBD) FENDERS ARE DAMAGED.","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.28","Very High","","","REPAIRS CARRIED OUT FOR THE TIME BEING. REQUISITION RAISED FOR THE SAME AND AWAITING FOR SPARES.","2023-03-25T23:59:35","DPEO230050","Completed","2023-01-09T23:59:35","No","No","No","Internal"]
[null,null,null,28708,95260,"0_Mon Jan 30 2023 15:46:52 GMT+0800","2023-01-13T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Stripper pump stroke counter gives erratic reading, Investigation required.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.15","High","","","Activated the stroke sensor and found working, To test during next usage of the pump.","2023-08-27T23:59:35","","Completed","2023-07-31T23:59:35","No","No","No","Internal"]
[null,null,null,28713,59005,"50_Wed Feb 01 2023 17:17:33 GMT+0800","2023-01-15T23:59:35","Defect","Ship Staff","Ship Staff Insp.","EGCS IS NOT FUNCTIONING ON AUTO MODE. PRESENTLY BEING OPERATED IN MANUAL MODE SEQUENTIALLY OPERATING ALL THE PUMPS AND VALVES MANUALLY FROM THE REMOTE PANEL.","Elect. Mach. & Equip.","MARPOL Related","Equipment Related","10.32","Very High","","","TROUBLESHOOTING CARRIED OUT.FOUND THE AUTO SEQUENCE WAS GETTNG INTERRUPTED BY THE MAINTENANCE REQUEST ALARM FOR THE EGCS SW SUPPLY PP NO3 PANEL COOLING FAN. SAME ALARM CLEARED/UPDATED ON THE MAINTENANCE REQUEST AS THE FAN WAS RENEWED ON JAN 2023(ROB-2 NOS). PRESENTLY EGCS WORKING ON AUTO MODE.","2023-04-15T23:59:35","","Completed","2023-02-04T23:59:35","No","No","No","Internal"]
[null,null,null,28714,40823,"50_Wed Feb 01 2023 17:24:46 GMT+0800","2023-01-15T23:59:35","Defect","Ship Staff","Ship Staff Insp.","ENGINE ROOM SERVICE AIR COMPRESSOR (ATLAS COPCO/SCREW COMPRESSOR) TRIPPING ON HIGH TEMPERATURE ALARM","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Presently working satisfactorily after oil change. Recommend to renew with atlas copco oil.","2023-04-15T23:59:35","","Completed","2023-04-05T23:59:35","No","No","No","Internal"]
[null,null,null,28715,20316,"50_Wed Feb 01 2023 17:29:42 GMT+0800","2023-01-15T23:59:35","Defect","Ship Staff","Ship Staff Insp.","BILGE PUMP IS UNABLE TO TAKE SUCTION FROM THE BILGE WELLS","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","FAULT FINDING/TROUBLESHOOTING CARRIED OUT. BILGE LINE SUCTION VALVE AND PORT BILGE WELL SUCTION VALVE OVERHAULED. TIRED OUT BILGE PUMP FROM ALL BILGE WELLS NOW WORKING SATISFACTORILY.","2023-04-15T23:59:35","","Completed","2023-02-04T23:59:35","No","No","No","Internal"]
[null,null,null,34716,47469,"50_Tue Mar 26 2024 16:54:46 GMT+0800","2023-01-15T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Deck air compressor delivery side flexible hose leaking.","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related","","","","","Deck Air compressor  Delivery side flexible air hose  change.","2024-07-13T23:59:35","DPEO240031","Completed","2024-07-15T23:59:35","No","No","No","Internal"]
[null,null,null,28709,13967,"50_Mon Jan 30 2023 15:55:01 GMT+0800","2023-01-24T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Brake levers of M1, M5 does not stay in open position.\nM2 winch hydarulic brake non-operational. Same have to be used in manual mode.","Deck - Machinery","Mooring","Equipment Related","9.14","Medium","","","Brake lever overhauled and made operational.","2023-03-24T23:59:35","","Completed","2023-02-12T23:59:35","No","No","No","Internal"]
[null,null,null,28710,96536,"50_Mon Jan 30 2023 15:59:44 GMT+0800","2023-01-24T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Both provision crane  hook runner limit switches non-operational.","Deck - Machinery","Mooring","Equipment Related","8.50","Medium","","","Both provision crane hook runner limit switches cam adjusted. Presently working satisfactorily.","2023-03-25T23:59:35","","Completed","2023-02-10T23:59:35","No","No","No","Internal"]
[null,null,null,28697,87378,"50_Mon Jan 30 2023 08:13:11 GMT+0800","2023-01-25T23:59:35","Other","Ship Staff","Ship Staff Insp.","No.2 Gyro annual due on 06 Feb 2023.","Navigation - Others","Navigation","Equipment Related","","","","","Annual servicing carried out.","2023-02-01T23:59:35","","Completed","2023-03-17T23:59:35","No","No","No","Internal"]
[null,null,null,28698,46433,"50_Mon Jan 30 2023 08:17:42 GMT+0800","2023-01-25T23:59:35","Other","Ship Staff","Ship Staff Insp.","Navtex printer giving faded prints.","Navigation - GMDSS & Communication,Navigation - Others","Navigation","Equipment Related","","","","","Renewed printer from spare","2023-02-24T23:59:35","DPEO220300","Completed","2023-03-24T23:59:35","No","No","No","Internal"]
[null,null,null,28699,42988,"50_Mon Jan 30 2023 08:20:30 GMT+0800","2023-01-25T23:59:35","Critical Equipment","Ship Staff","Ship Staff Insp.","ECDIS annual shore servicing required, as Navtex messages are not automatically plotting on both ECDIS. This function was active earlier","Navigation - ECDIS","Navigation","Equipment Related","","","","","ECDIS service engineer came at Singapore on 21 May 2023, the problem resolved, Navtex messages getting auto plot on ECDIS","2023-05-26T23:59:35","","Completed","2023-05-18T23:59:35","No","No","No","Internal"]
[null,null,null,28700,47481,"50_Mon Jan 30 2023 08:24:47 GMT+0800","2023-01-25T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Doppler log, STBD bridge wing repeater digital display faded/incomplete.","Navigation - Echo Sounder / Speed Log","Navigation","Equipment Related","","","","","Requisition raised, awaiting for supply","2023-05-25T23:59:35","DPEO230052","Completed","2023-03-21T23:59:35","No","No","No","Internal"]
[null,null,null,28701,50291,"50_Mon Jan 30 2023 09:32:30 GMT+0800","2023-01-25T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Bridge center window wiper belt broken","Accommodation","Navigation","Equipment Related","","","","","Wiper belt replaced. Wiper is operational now. Requisition raised for new spare parts","2023-03-26T23:59:35","","Completed","2023-02-25T23:59:35","No","No","No","Internal"]
[null,null,null,29467,19426,"50_Mon Feb 27 2023 13:24:17 GMT+0800","2023-01-27T23:59:35","Defect","Ship Staff","Ship Staff Insp.","TGE UNIT OF CARGO TANK NON-OPERATIONAL","Critical Equip.","","Equipment Related","8.19","High","","","Renewed from spare.","2023-05-26T23:59:35","DPEO230022","Completed","2023-03-26T23:59:35","No","No","No","Internal"]
[null,null,null,29475,33483,"50_Thu Feb 09 2023 15:28:31 GMT+0800","2023-02-03T23:59:35","Defect","Ship Staff","Ship Staff Insp.","ME FO heater NO#2 leaks observed from both fuel and water side end covers.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Renewed the gaskets by opening the end cover and arresting the leak.","2023-06-03T23:59:35","","Completed","2023-05-08T23:59:35","No","No","No","Internal"]
[null,null,null,29482,42201,"50_Mon Mar 20 2023 09:21:39 GMT+0800","2023-02-14T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","#2 LO purifier not operational.Bowl leaking.","E/R - Purifier","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Working satisfactorily.","2023-06-27T23:59:35","","Completed","2023-06-17T23:59:35","No","No","No","Internal"]
[null,null,null,29471,38859,"50_Wed Mar 15 2023 13:52:49 GMT+0800","2023-02-24T23:59:35","Defect","Ship Staff","Ship Staff Insp.","RUDDER CARRIER GRESSE PUMP NOT RUNNING IN AUTO MODE","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Added stop timer and found working in auto Twice a day for 10seconds.","2023-07-26T23:59:35","DPEO230196","Completed","2023-06-14T23:59:35","No","No","No","Internal"]
[null,null,null,29472,53101,"50_Thu Mar 16 2023 09:12:54 GMT+0800","2023-02-24T23:59:35","Defect","Ship Staff","Ship Staff Insp.","STEAM LEAK OBSERVED FROM 7K SERVICE LINE WHICH IS AT A HEIGHT OF 10 M FROM PLATFORM LEVEL ABOVE THE BOILER BURNER AND DOES NOT HAVE ANY ACCESS AND NO PROPER/FLAT FOUNDATION FOR LAYING LADDER.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Behaviour Based","10.32","Very High","","","TIGHTENED ALL BOLTS AND CHECKED FOR LEAKS FOUND HOLDING GOOD.","2023-06-26T23:59:35","","Completed","2023-03-26T23:59:35","No","No","No","Internal"]
[null,null,null,29473,17768,"50_Thu Mar 16 2023 09:22:16 GMT+0800","2023-02-24T23:59:35","Defect","Ship Staff","Ship Staff Insp.","AFT LT COOLER ALL INLET AND OUTLET VALVES (4 NOS) VALVES NOT HOLDING.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Behaviour Based","10.32","Very High","","","Inlet valve renewed from spare. Outlet valve found to be shifted by 180degrees same placed correctly and tried out found holding good.","2023-06-26T23:59:35","DPEO230106","Completed","2023-03-25T23:59:35","No","No","No","Internal"]
[null,null,null,29474,96053,"50_Thu Mar 16 2023 09:28:45 GMT+0800","2023-02-24T23:59:35","Other","Ship Staff","Ship Staff Insp.","HIGH SEA CHEST INLET VALVE ARE NOT HYDRAULIC. IT IS A NORMAL VALVE","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","ADDED IN REFMAN TO BE DONE IN DD JOB NO.74","2023-07-26T23:59:35","","Completed","2023-06-15T23:59:35","No","No","No","Internal"]
[null,null,null,29476,22993,"50_Thu Mar 16 2023 09:30:18 GMT+0800","2023-02-24T23:59:35","Other","Ship Staff","Ship Staff Insp.","EGCS SEA CHEST INLET  VALVE DOES NOT HAVE HYDRAULIC ACTUATOR ","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","ADDED IN REFMAN JOB NO.75","2023-07-26T23:59:35","","Completed","2023-06-15T23:59:35","No","No","No","Internal"]
[null,null,null,29477,14274,"50_Thu Mar 16 2023 09:36:40 GMT+0800","2023-02-24T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","ACCOMMODATION AIR CONDITIONING SYSTEM #1 DRIER INLET VALVE (CONDENSER OUTLET VALVE)  NOT HOLDING AND HAVE  LEAKS FROM VARIOUS LOCATIONS IN THE SYSTEM","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","leaks rectified","2023-08-26T23:59:35","DPEO230176","Completed","2023-07-17T23:59:35","No","No","No","Internal"]
[null,null,null,29468,50064,"50_Wed Mar 15 2023 11:55:34 GMT+0800","2023-03-05T23:59:35","Defect","Ship Staff","Ship Staff Insp.","salinometer showing wrong value, checked the sensor found all the terminals for the sensor in brittle and broken condition.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","Renewed and tried out found working satisfactorily.","2023-07-26T23:59:35","DPEO230135","Completed","2023-03-26T23:59:35","No","No","No","Internal"]
[null,null,null,29479,14579,"50_Sun Mar 19 2023 16:41:36 GMT+0800","2023-03-07T23:59:35","Defect","Ship Staff","Ship Staff Insp.","ICO LUB SYSTEM AUTO MIXING PROGRAM (CYLINDER OIL:ME SUMP OIL)GIVING FAULT ALARM.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Presently found working satisfactorily.","2023-07-07T23:59:35","","Completed","2023-06-04T23:59:35","No","No","No","Internal"]
[null,null,null,29478,80435,"50_Sun Mar 19 2023 14:32:18 GMT+0800","2023-03-12T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Aux boiler #2 Outlet from EGB inlet to the boiler valve not holding. Level float chamber steam valves not holding","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Valve overhauled and put in operation, presently no leaks.","2023-07-12T23:59:35","DPEO230194","Completed","2023-06-08T23:59:35","No","No","No","Internal"]
[null,null,null,29481,99003,"50_Mon Mar 20 2023 09:18:48 GMT+0800","2023-03-14T23:59:35","Defect","Ship Staff","Ship Staff Insp.","#2 LO purifier motor ammeter not working.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Checked connections for tightness found working","2023-07-14T23:59:35","","Completed","2023-05-09T23:59:35","No","No","No","Internal"]
[null,null,null,29480,30732,"50_Mon Mar 20 2023 09:15:45 GMT+0800","2023-03-15T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Sewage treatment plant settling tank suction vv stuck in closed position.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Fabricated new spindle and tried out found working satisfactory.","2023-07-15T23:59:35","","Completed","2023-05-23T23:59:35","No","No","No","Internal"]
[null,null,null,29917,12392,"50_Sat Apr 01 2023 12:08:48 GMT+0800","2023-03-17T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Aft most bulkhead of engine casing on poop deck to clean and paint","Miscellaneous","General Appearance","External Factors","","","","","Aft most said bulkhead cleaned and painted","2023-05-27T23:59:35","","Completed","2023-05-22T23:59:35","No","No","No","Internal"]
[null,null,null,29918,29922,"50_Sat Apr 01 2023 12:12:23 GMT+0800","2023-03-17T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Main deck hydraulic boxed to derust and paint","Miscellaneous","General Appearance","External Factors","","","",""," derust and painted","2023-08-27T23:59:35","","Completed","2023-07-19T23:59:35","No","No","No","Internal"]
[null,null,null,29921,68809,"50_Sat Apr 01 2023 12:06:13 GMT+0800","2023-03-17T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Engine room funnel to paint at anchorage.","Miscellaneous","General Appearance","External Factors","","","","","All funnel stacks and funnel painted","2023-05-27T23:59:35","","Completed","2023-05-28T23:59:35","No","No","No","Internal"]
[null,null,null,29929,87857,"50_Fri Mar 31 2023 19:22:43 GMT+0800","2023-03-17T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Engine room toilet flush not operational and toilet in dirty condition.","Miscellaneous","Eng. / Strg. Comp.","Human Error","11.13","Low","","","cleaned","2023-03-27T23:59:35","","Completed","2023-03-27T23:59:35","No","No","No","Internal"]
[null,null,null,29930,99693,"50_Fri Mar 31 2023 19:27:49 GMT+0800","2023-03-17T23:59:35","Critical Equipment","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Port lifeboat motor found tripping in high speed mode while hoisting.","LSA / FFA","Emgcy. Systems","Equipment Related","5.15","Medium","","","Inspected the circuit and renewed the starter. Presently working satisfactory.","2023-03-24T23:59:35","","Completed","2023-03-27T23:59:35","No","No","No","Internal"]
[null,null,null,29931,51088,"50_Sat Apr 01 2023 12:10:32 GMT+0800","2023-03-17T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Paint found peeling on the way of the mooring wires on deck","Miscellaneous","General Appearance","External Factors","","","","","Removed the peeled area, cleaned, buffed and painting carried out.","2023-04-07T23:59:35","","Completed","2023-03-27T23:59:35","No","No","No","Internal"]
[null,null,null,29932,29059,"50_Fri Mar 31 2023 19:36:10 GMT+0800","2023-03-17T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Oily rags and oily buckets lying in garbage locker","Miscellaneous","General Appearance","Human Error","6.20","Medium","","","Arranged, cleaned and painted.","2023-03-30T23:59:35","","Completed","2023-03-27T23:59:35","No","No","No","Internal"]
[null,null,null,29933,72987,"50_Fri Mar 31 2023 19:39:23 GMT+0800","2023-03-17T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","STBD Windlass gear case oil found emulsified.","Deck - Machinery","Mooring","Equipment Related","9.14","Medium","","","OIL RENEWED AND NEW SIGHT GLASS INSTALLED","2023-03-31T23:59:35","","Completed","2023-03-30T23:59:35","No","No","No","Internal"]
[null,null,null,29934,94462,"50_Fri Mar 31 2023 19:25:57 GMT+0800","2023-03-17T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Elevator light fitting to renew and floor mat to change to green","Accommodation","General Appearance","External Factors","11.16","Low","","","Renewed the floor mat, renewed the light.","2023-03-30T23:59:35","","Completed","2023-03-30T23:59:35","No","No","No","Internal"]
[null,null,null,29936,77517,"50_Fri Mar 31 2023 19:24:14 GMT+0800","2023-03-17T23:59:35","Defect,Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","HP Boiler circulating pump oil pot was empty.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Modified and made the seal pot operational.","2023-03-30T23:59:35","","Completed","2023-04-07T23:59:35","No","No","No","Internal"]
[null,null,null,29938,67165,"50_Fri Mar 31 2023 19:31:56 GMT+0800","2023-03-17T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Leakage reported from STBD Air con. unit","Accommodation,Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Renewed the mechanical seal, pressure tested the compressor and arrested all leaks.","2023-04-17T23:59:35","","Completed","2023-04-17T23:59:35","No","No","No","Internal"]
[null,null,null,29939,75584,"50_Sun Apr 16 2023 00:47:34 GMT+0800","2023-03-18T23:59:35","Defect","Ship Staff","Ship Staff Insp.","During Lub oil bunkering at Singapore observed leak in M/E LO bunker line. To renew the pipeline.","Deck - Pipe / Fittings","Eng. / Strg. Comp.","Equipment Related,External Factors","11.5","Medium","","","Renewed the pipeline, pressure tested found in good condition.","2023-04-26T23:59:35","","Completed","2023-04-04T23:59:35","No","No","No","Internal"]
[null,null,null,29935,36210,"50_Sun Apr 16 2023 00:43:37 GMT+0800","2023-03-28T23:59:35","Defect","Ship Staff","Ship Staff Insp.","EGB Pump pressure switch is defective, needs renewal. To check and raise requisition for the same.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Renewed with spare M/E Pressure sensor and tried out found working satisfactorily.","2023-06-05T23:59:35","","Completed","2023-04-09T23:59:35","No","No","No","Internal"]
[null,null,null,29920,90627,"50_Sun Apr 16 2023 00:52:56 GMT+0800","2023-04-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Scavenge pressure alarm exist in the NABTESCO control panel after EPL Installation.","E/R - Main Engine","Eng. / Strg. Comp.","External Factors","10.32","Very High","","","Wartsila and Nabtesco Service Engineers attended and solve the issue by calibration of Load indicator #1 and #2. Adjusted 4~20mA = 0% ~ 100%\nAdjusted TK: 730 ~ Tk: 734, 715 ~ 719. Pls see Service Report dated 20-Oct-2023.","2023-09-19T23:59:35","","Completed","2023-10-20T23:59:35","No","No","No","Internal"]
[null,null,null,29923,10701,"50_Sun Apr 16 2023 00:56:31 GMT+0800","2023-04-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","The CEMS Reading is not being displayed in the ECR SOX Scrubber panel.","E/R - Aux. Mach.","Eng. / Strg. Comp.","External Factors","10.32","Very High","","","SICK Service Engineer attended in Singapore Anchorage CEMS communication with the MCP HMI has been resolved. Please see Service Report dated 19-Oct-2023 for complete job details carried out.","2023-09-19T23:59:35","","Completed","2023-10-19T23:59:35","No","No","No","Internal"]
[null,null,null,29924,99170,"50_Sun Apr 16 2023 00:58:00 GMT+0800","2023-04-01T23:59:35","Defect,Observation","Ship Staff","Ship Staff Insp.","EGB Sootblowing not carried out for a long time","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Overhauled and put in use.","2023-06-17T23:59:35","","Completed","2023-06-18T23:59:35","No","No","No","Internal"]
[null,null,null,29937,66058,"50_Sun Apr 16 2023 01:22:05 GMT+0800","2023-04-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Bilges being transfered by external means due to leaky Port bilge well valve.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","External Factors","10.32","Very High","","","Renewed the valve and tried out found working satisfactorily.","2023-06-12T23:59:35","","Completed","2023-04-12T23:59:35","No","No","No","Internal"]
[null,null,null,29919,14557,"50_Sat Apr 15 2023 20:19:54 GMT+0800","2023-04-04T23:59:35","Observation","Ship Staff","Ship Staff Insp.","SUSPECT MASTRISER BREATHER VALVE LEAKING","Inert Gas","Cargo / Ballast Systems","Equipment Related","","","","","Mastriser valve observed not closing completely due to stopper nuts on gear box assembly, same adjusted, mastriser valve is closing completely and no leak is observed now.","2023-05-27T23:59:35","","Completed","2023-06-02T23:59:35","No","No","No","Internal"]
[null,null,null,29926,38458,"50_Mon May 01 2023 10:01:34 GMT+0800","2023-04-12T23:59:35","Observation","Ship Staff","Ship Staff Insp.","ME Unit no.2 Quills found leaking off water.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Overhauled the unit and renewed liner and tried out found no leaks.","2023-06-26T23:59:35","","Completed","2023-05-20T23:59:35","No","No","No","Internal"]
[null,null,null,29925,63700,"50_Mon May 01 2023 09:59:38 GMT+0800","2023-04-13T23:59:35","Observation","Ship Staff","Ship Staff Insp.","STBD LIFEBOAT SPRINKER PUMP BASE IS FOUND BROKEN","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.28","Very High","","","Renewed the pump and tried out working satisfactorily.","2023-07-11T23:59:35","DPEO230158","Completed","2023-06-17T23:59:35","No","No","No","Internal"]
[null,null,null,29927,37365,"50_Mon May 01 2023 20:22:56 GMT+0800","2023-04-20T23:59:35","Defect","Ship Staff","Ship Staff Insp.","No.1 & 2 Ballast pump Lower bearing temperature sensor is not working.","Deck - Machinery","Cargo / Ballast Systems","Equipment Related","8.19","High","","","New spares received and installed. Checked and verify the temperature found all matching.","2023-07-19T23:59:35","DPEO230152","Completed","2023-08-08T23:59:35","No","No","No","Internal"]
[null,null,null,30000,39945,"50_Mon May 15 2023 09:21:19 GMT+0800","2023-04-29T23:59:35","Defect","Ship Staff","Ship Staff Insp.","COPT Condenser pump not working due to leakage from mechanical seal.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Renewed the shaft seal and tried out found working satisfactory.","2023-07-12T23:59:35","","Completed","2023-05-14T23:59:35","No","No","No","Internal"]
[null,null,null,30001,33743,"50_Mon May 15 2023 09:22:44 GMT+0800","2023-04-30T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Control air dryer for E/R BWTS air supply is leaking","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Cleaned the drain tried out found no leaks and working satisfactorily.","2023-08-12T23:59:35","","Completed","2023-06-01T23:59:35","No","No","No","Internal"]
[null,null,null,30002,70956,"50_Wed May 17 2023 07:55:49 GMT+0800","2023-05-12T23:59:35","Observation","Ship Staff","Ship Staff Insp.","In 2 Stbd WBT, 1 number U clamp bend, same to be opened straightened and fix back in place","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","","","","","U CLAMP RENEWED IN 2 STBD WBT","2023-08-27T23:59:35","","Completed","2023-07-06T23:59:35","No","No","No","Internal"]
[null,null,null,30352,98047,"50_Sun Jun 04 2023 14:19:03 GMT+0800","2023-05-15T23:59:35","Defect","Ship Staff","Ship Staff Insp.","No.1 EGCS water pump panel cooling fan not working","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","new Panel AC installed ","2023-08-14T23:59:35","DPEO230170","Completed","2023-07-09T23:59:35","No","No","No","Internal"]
[null,null,null,30503,11690,"50_Sat Jun 17 2023 20:12:16 GMT+0800","2023-05-26T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","No 3 DG FCU high temp , low temp and low visc alarm active. To trouble shoot and rectify","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Cleaned the sensor found the Viscosense working satisfactory.","2023-09-26T23:59:35","DPEO230230","Completed","2023-10-10T23:59:35","No","No","No","Internal"]
[null,null,null,30504,98150,"50_Sat Jun 17 2023 20:13:54 GMT+0800","2023-05-26T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Duct in China Passage to repair and paint.","Deck - Pipe / Fittings","General Appearance","External Factors","11.5","Medium","","","Duct in China Passage to repaired and painted.","2023-12-15T23:59:35","","Completed","2023-11-14T23:59:35","No","No","No","Internal"]
[null,null,null,30505,38817,"50_Sat Jun 17 2023 20:17:56 GMT+0800","2023-05-26T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Dedicated wooded box to fabricate for Aldis lamp on bridge.","Navigation - Others","General Appearance","External Factors","","","","","DEDICATED WOODEN BOX FABRICATED FOR ALDIS LAMP ON BRIDGE","2023-07-27T23:59:35","","Completed","2023-07-14T23:59:35","No","No","No","Internal"]
[null,null,null,30506,69059,"50_Sat Jun 17 2023 20:24:02 GMT+0800","2023-05-26T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Both Lifeboat embarkation plate stiffner to renew as same in corroded condition.","Deck - Machinery,Deck - Pipe / Fittings","Structural Condn. / WT integrity ","External Factors","11.5","Medium","","","To derust and check the condition and renew as necessary.\n\nBoth Lifeboat embarkation plate stiffners de-rusted and painted. Cold work carried out","2024-02-29T23:59:35","","Completed","2024-02-26T23:59:35","No","No","No","Internal"]
[null,null,null,30508,35020,"50_Sat Jun 17 2023 20:27:03 GMT+0800","2023-05-26T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","On Main deck many of the hydraulic boxes protection plates to renew, as same found in corroded condition.","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","External Factors","11.5","Medium","","","3 NOS HYDRAULIC BOX PROTECTION PLATE REMOVED, TAKEN TO E/R WORKSHOP. WASTE DSECTION RENEWED, PLATE DERUSTED AND PAINTED. SAME FIXED BACK IN PLACE. WORK COMPLETED","2023-08-12T23:59:35","","Completed","2023-07-10T23:59:35","No","No","No","Internal"]
[null,null,null,30509,62557,"50_Sat Jun 17 2023 20:28:04 GMT+0800","2023-05-26T23:59:35","Non Conformity,Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Manifold area below pipelines to paint.","Deck - Pipe / Fittings","General Appearance","External Factors","11.5","Medium","","","to derust and paint.\n\nPainting carried out","2024-05-08T23:59:35","","Completed","2024-04-16T23:59:35","No","No","No","Internal"]
[null,null,null,30511,96065,"50_Sat Jun 17 2023 20:34:00 GMT+0800","2023-05-26T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Many of the winch gear oil is dirty or emulsified. TO renew the oil.","Deck - Mooring Machinery","Mooring","Human Error","9.14","Medium","","","ENCLOSED GEAR OIL REPLACED AND SIGHT GLASS RENEWED FOR ALL MOORING WINCHES AND WINDLASS","2023-08-12T23:59:35","","Completed","2023-07-06T23:59:35","No","No","No","Internal"]
[null,null,null,30512,63442,"50_Sat Jun 17 2023 20:36:32 GMT+0800","2023-05-26T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Fwd hydraulic motor no 1 and no 3 motor coupling is missing. To replace.","Deck - Mooring Machinery","Mooring","External Factors","10.32","Very High","","","motor coupling renewed.","2024-06-15T23:59:35","DPEO230219","Completed","2024-06-06T23:59:35","No","No","No","Internal"]
[null,null,null,30513,70178,"50_Sat Jun 17 2023 20:22:21 GMT+0800","2023-05-26T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Lifeboat Greasing points to highlight in yellow.","Deck - Machinery","General Appearance","External Factors","","","","","BOTH LIFEBOAT PORT AND STBD DAVIT ALL GREASE POINTS HIGHLIGHTED IN YELLOW","2023-07-12T23:59:35","","Completed","2023-06-19T23:59:35","No","No","No","Internal"]
[null,null,null,30514,72238,"50_Sat Jun 17 2023 20:21:15 GMT+0800","2023-05-26T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","No 3 COP vibration alarm active even in stop condition to rectify.","Deck - Machinery","Cargo / Ballast Systems","Equipment Related","8.80","Medium","","","Checked the supports tightness. Presently no alarm, to be checked during trial. Found not activating during the Pressure testing of COP.","2023-09-27T23:59:35","","Completed","2023-10-17T23:59:35","No","No","No","Internal"]
[null,null,null,30515,41332,"50_Sat Jun 17 2023 20:37:27 GMT+0800","2023-05-26T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ETA Box light broken. To replace.","Deck - Pipe / Fittings","General Appearance","External Factors","","","","","Replaced with New recvd SI light","2023-06-27T23:59:35","","Completed","2023-07-02T23:59:35","No","No","No","Internal"]
[null,null,null,30516,31546,"50_Sat Jun 17 2023 20:38:41 GMT+0800","2023-05-26T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","EGCS room louvre wheel found seized","Deck - Pipe / Fittings","Eng. / Strg. Comp.","External Factors","11.6","Medium","","","Derusted, painted and eased up for easy operation.","2023-06-27T23:59:35","","Completed","2023-06-21T23:59:35","No","No","No","Internal"]
[null,null,null,30517,37376,"50_Sat Jun 17 2023 20:40:15 GMT+0800","2023-05-26T23:59:35","Critical Equipment","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Emergency DG frequency found hunting while running in idle condition. To check and adjust.","LSA / FFA","Emgcy. Systems","Equipment Related","10.32","Very High","","","Tightened governor screw by the droop setting, hunting issue resolved.","2023-09-24T23:59:35","","Completed","2023-09-27T23:59:35","No","No","No","Internal"]
[null,null,null,30518,53428,"50_Sat Jun 17 2023 20:41:11 GMT+0800","2023-05-26T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Emergency DG room shore cable opening cover rusted and distorted. To renew.","Deck - Pipe / Fittings","General Appearance","External Factors","11.6","Medium","","","cover renewed. ","2023-07-19T23:59:35","","Completed","2023-07-19T23:59:35","No","No","No","Internal"]
[null,null,null,30519,20395,"50_Sat Jun 17 2023 20:44:36 GMT+0800","2023-05-26T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","File Management System to update.","Miscellaneous","ISM Related","Industry Issue","","","","","JOB COMPLETED","2023-06-27T23:59:35","","Completed","2023-07-02T23:59:35","No","No","No","Internal"]
[null,null,null,30520,35004,"50_Sat Jun 17 2023 20:16:48 GMT+0800","2023-05-26T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Hydraulic hoses in common store to shift to Steering gear room with proper storage arrangement.","Miscellaneous","General Appearance","External Factors","10.32","Very High","","","kept a space in racks for the hydraulic hoses and shifted to steering gear room.","2023-06-12T23:59:35","","Completed","2023-06-04T23:59:35","No","No","No","Internal"]
[null,null,null,30962,47778,"50_Thu Jun 29 2023 20:40:13 GMT+0800","2023-06-23T23:59:35","Observation","Ship Staff","Ship Staff Insp.","The drain pot of A/E no.3 air cooler drain to be removed and Ball valve to be put in place.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","",""," Removed the drain pot and installed a ball valve in place and tried out the A/E 3.","2023-09-22T23:59:35","","Completed","2023-07-02T23:59:35","No","No","No","Internal"]
[null,null,null,31694,23204,"50_Tue Aug 15 2023 08:45:29 GMT+0800","2023-08-01T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Torn lagging on pipeline on top of Aux boiler","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","External Factors","10.32","Very High","","","Steam line laggings renewed along the  top of the Boiler before the vetting inspection.","2023-09-19T23:59:35","","Completed","2023-09-29T23:59:35","No","No","No","Internal"]
[null,null,null,31695,74242,"50_Fri Aug 18 2023 00:00:29 GMT+0800","2023-08-01T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Leak near EGCS S/W Pump discharge line temporarily arrested.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","EGCS S/W Pumps discharge common manifold line removed from place and reapired in workshop means of steel plate insert welding.","2023-11-30T23:59:35","","Completed","2023-12-31T23:59:35","No","No","No","Internal"]
[null,null,null,31696,50927,"50_Sat Aug 19 2023 09:52:37 GMT+0800","2023-08-01T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Stbd MOB Cradle corroded and holed","LSA / FFA","Structural Condn. / WT integrity ","Equipment Related","5.31","High","","","MOB cradle to be cropped and renewed","2024-01-15T23:59:35","","Completed","2024-01-05T23:59:35","No","No","No","Internal"]
[null,null,null,31697,74398,"50_Sat Aug 19 2023 10:04:45 GMT+0800","2023-08-01T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Many exterior light fittings base heavily corroded and wasted.","Deck - Pipe / Fittings","General Appearance","External Factors","11.9","Low","","","Light fittings   cropped and renewed","2023-09-17T23:59:35","","Completed","2023-09-08T23:59:35","No","No","No","Internal"]
[null,null,null,31698,70378,"50_Sat Aug 19 2023 10:09:07 GMT+0800","2023-08-01T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Scrubber tower entrance and pipeline near the entrance rusted","Accommodation","General Appearance","External Factors","11.13","Low","","","Scrubber tower entrance and pipeline to be de-rusted and painting completed before vetting inspection.","2023-09-16T23:59:35","","Completed","2023-09-29T23:59:35","No","No","No","Internal"]
[null,null,null,31699,22542,"50_Sat Aug 19 2023 10:11:39 GMT+0800","2023-08-01T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Base plate of PA Speaker at accommodation exterior corroded and wasted.","Accommodation","General Appearance","Equipment Related","11.13","Low","","","Base plate of PA Speaker at accommodation exterior to be cropped and renewed","2024-06-15T23:59:35","","Completed","2024-06-10T23:59:35","No","No","No","Internal"]
[null,null,null,31700,35832,"50_Fri Aug 18 2023 00:12:20 GMT+0800","2023-08-01T23:59:35","Defect,Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Pin hole leak on IG Scrubber overboard line.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Pipeline hot work repair carried out by placing an insert  .","2023-11-30T23:59:35","","Completed","2023-09-20T23:59:35","No","No","No","Internal"]
[null,null,null,31701,75137,"50_Sat Aug 19 2023 10:25:19 GMT+0800","2023-08-01T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","‘B’ Deck portside exterior accommodation deck rusted.","Accommodation","General Appearance","External Factors","11.1","High","","","‘B’ Deck portside exterior accommodation deck  derusted and painted","2023-09-17T23:59:35","","Completed","2023-09-16T23:59:35","No","No","No","Internal"]
[null,null,null,31702,26143,"50_Sat Aug 19 2023 10:31:44 GMT+0800","2023-08-01T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Engine room air intake on funnel deck rusted and have weeping marks.","Miscellaneous","","Equipment Related","11.1","High","","","Engine room air intake on funnel deck de-rusted and painting completed before vetting inspection.","2023-10-01T23:59:35","","Completed","2023-09-29T23:59:35","No","No","No","Internal"]
[null,null,null,31703,61147,"50_Sat Aug 19 2023 10:57:31 GMT+0800","2023-08-01T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Supports for air duct of Galley exhaust and supply blowers heavily wasted and broken.","Accommodation","General Appearance","Equipment Related","11.13","Low","","","Supports for air duct of Galley exhaust and supply blowers cropped and renewed","2023-12-30T23:59:35","","Completed","2023-11-17T23:59:35","No","No","No","Internal"]
[null,null,null,31704,44636,"50_Sat Aug 19 2023 11:04:40 GMT+0800","2023-08-01T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Manholes of Ballast tanks, void spaces and Cargo tanks rusted at the borders near the bolts.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Inappropriate Procedure","11.7","High","","","Derusting and painting of ballast tank manholes, void spaces and cargo tanks is completed.","2024-08-15T23:59:35","","Completed","2024-07-31T23:59:35","No","No","No","Internal"]
[null,null,null,31705,62378,"50_Sat Aug 19 2023 11:12:07 GMT+0800","2023-08-01T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Deck store entrance base plated corroded and wasted.","Accommodation","General Appearance","Inappropriate Procedure","11.6","Medium","","","Deck store entrance base plated  derusted and painted","2023-10-01T23:59:35","","Completed","2023-08-10T23:59:35","No","No","No","Internal"]
[null,null,null,31706,35609,"50_Sat Aug 19 2023 10:19:57 GMT+0800","2023-08-01T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Port and Stbd provision crane rusted and having weeping marks","Deck - Machinery","General Appearance","Equipment Related","","","","","Rusted areas of Port and Stbd provision crane to be derusted and painted.\n\nPort and starboard provision cranes de-rusted and painted","2024-03-29T23:59:35","","Completed","2024-02-19T23:59:35","No","No","No","Internal"]
[null,null,null,31707,78205,"50_Sat Aug 19 2023 11:32:20 GMT+0800","2023-08-01T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","IG Branch Valves rusted and require cosmetic upgradation.","Cargo Mach.,Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","11.1","High","","","IG Branch Valves derusting and  painting in progress","2024-05-31T23:59:35","","Completed",null,"No","No","No","Internal"]
[null,null,null,31708,98071,"50_Sat Aug 19 2023 11:16:43 GMT+0800","2023-08-01T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Weeping marks and rust stains on accommodation at various locations.","Accommodation","General Appearance","Inappropriate Procedure","11.1","High","","","Weeping marks and rust stains on accommodation cleaned. Derusting and painting of spot areas to be carried out","2024-04-09T23:59:35","","Completed","2024-03-18T23:59:35","No","No","No","Internal"]
[null,null,null,31709,86561,"50_Sat Aug 19 2023 11:28:14 GMT+0800","2023-08-01T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Vents around accommodation and funnel deck rusted.","Accommodation","General Appearance","Equipment Related","11.13","Low","","","Vents around accommodation and funnel deck washed and cleaned. De-rusting and Painting in completed.","2023-09-17T23:59:35","","Completed","2023-09-29T23:59:35","No","No","No","Internal"]
[null,null,null,31710,32439,"50_Sat Aug 19 2023 11:27:03 GMT+0800","2023-08-01T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","T/C air intake on funnel deck rusted and have weeping marks","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.1","High","","","T/C air intake on funnel deck de-rusted and painting completed.","2023-10-08T23:59:35","","Completed","2023-09-29T23:59:35","No","No","No","Internal"]
[null,null,null,31711,88973,"50_Sat Aug 19 2023 11:41:54 GMT+0800","2023-08-01T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Hissing leaking sound from 1C P/V Valve. To be investigated further.","Deck - Pipe / Fittings","Cargo / Ballast Systems","External Factors","8.41","Medium","","","Hissing leaking sound from 1C P/V Valve to be checked and further\nPV valves inspected observed  O-ring/ Seal ring  is getting torn and damaged at places causing slight leakages in P/V valves.\nRequested Office on query to order the same, as not mentioned in the manual.\nManual received, PO DPEO230344 raised, awaiting spares.\n\nAll PV valves lip seals renewed.\n","2024-02-29T23:59:35","DPEO230344","Completed","2024-02-12T23:59:35","No","No","No","Internal"]
[null,null,null,31712,88937,"50_Sat Aug 19 2023 11:52:33 GMT+0800","2023-08-01T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Vapour return line having rust spots at various locations","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","11.1","High","","","Vapour return line to be spot derusted and painted","2024-04-09T23:59:35","","Completed","2024-04-05T23:59:35","No","No","No","Internal"]
[null,null,null,31713,84712,"50_Sat Aug 19 2023 11:54:00 GMT+0800","2023-08-01T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Cargo manifold lines having rust spots at various locations.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","11.1","High","","","Cargo manifold lines de rusting and painting completed. ","2024-10-31T23:59:35","","Completed","2024-08-17T23:59:35","No","No","No","Internal"]
[null,null,null,29922,35609,"50_Sun Apr 16 2023 00:54:47 GMT+0800","2023-08-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","The M/E Load is not constant at the ECR Console, varies continuosily by 14 points.","E/R - Main Engine","Eng. / Strg. Comp.","External Factors","10.32","Very High","","","Wartsila and Nabtesco Service Engineers attended and solve the issue by calibration of Load indicator #1 and #2. Adjusted 4~20mA = 0% ~ 100%\nAdjusted TK: 730 ~ Tk: 734, 715 ~ 719. Pls see Service Report dated 20-Oct-2023.","2023-10-19T23:59:35","","Completed","2023-10-20T23:59:35","No","No","No","Internal"]
[null,null,null,31714,52368,"50_Sat Aug 19 2023 11:30:03 GMT+0800","2023-08-01T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Flanges and valves of pipelines on deck rusted and having weeping marks.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","11.1","High","","","Centre pipelines derusting and painting is completed.\nBranch piepelines and flanges derusting and painting in progress","2024-10-31T23:59:35","","Completed","2024-08-17T23:59:35","No","No","No","Internal"]
[null,null,null,31716,84000,"50_Sat Aug 19 2023 12:01:18 GMT+0800","2023-08-01T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Foam monitor platform and staircase having thick rust.","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.1","High","","","Foam monitor platform and staircase  de rusting and painting is completed.","2024-07-31T23:59:35","","Completed","2024-07-31T23:59:35","No","No","No","Internal"]
[null,null,null,31717,54160,"0_Sat Aug 19 2023 12:08:06 GMT+0800","2023-08-01T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","No 6B Hydraulic box on deck broken from hinges with oil sheen inside the box.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","6.9","Low","","","No 6B Hydraulic box on deck hinges renewal/ fabrication carried out.\n","2023-11-30T23:59:35","","Completed","2023-11-12T23:59:35","No","No","No","Internal"]
[null,null,null,31718,24044,"0_Sat Aug 19 2023 12:15:23 GMT+0800","2023-08-01T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Hydroblaster onboard is in operational and requires spares","Deck - Machinery","General Appearance","Equipment Related","10.12","Very High","","","Hydroblaster  spares  requisition raised DPEO230229.\nSpares received. Hydroblaster repaired and found working satisfactorily. ","2023-11-30T23:59:35","","Completed","2023-11-27T23:59:35","No","No","No","Internal"]
[null,null,null,31722,10886,"50_Tue Aug 15 2023 09:03:37 GMT+0800","2023-08-01T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Steering gear door not closing fully. Having gap at the base.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","5.35","Medium","","","Steering gear door was not closing fully due to uneven door packing. Door packing pressed and made even. and door is closing properly","2023-08-21T23:59:35","","Completed","2023-08-13T23:59:35","No","No","No","Internal"]
[null,null,null,31723,49354,"50_Tue Aug 15 2023 10:36:57 GMT+0800","2023-08-01T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Water leak at flange near transformers.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Heating steam line for AE3 FCU was leaking from flange, Isolated line and renewed the gasket.","2023-08-21T23:59:35","","Completed","2023-08-09T23:59:35","No","No","No","Internal"]
[null,null,null,31724,37209,"50_Wed Aug 16 2023 06:25:06 GMT+0800","2023-08-01T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Hot well lagging torn at one place and save all filled with water.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","In Save all water was collected due to flange leak of the filling line. Renewed gasket and leak rectified. Also repaired torn lagging. ","2023-08-31T23:59:35","","Completed","2023-08-09T23:59:35","No","No","No","Internal"]
[null,null,null,31725,49956,"50_Wed Aug 16 2023 06:41:43 GMT+0800","2023-08-01T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Lagging of Exhaust for No 2 Aux Engine loosely tied with seizing wire.","E/R - Aux. Engine","Eng. / Strg. Comp.","Human Error","10.32","Very High","","","No 2 Aux Engine turbocharger  lagging tied snugly and secured.","2023-08-21T23:59:35","","Completed","2023-08-07T23:59:35","No","No","No","Internal"]
[null,null,null,31726,65964,"50_Tue Aug 15 2023 07:08:32 GMT+0800","2023-08-01T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Oil leak near no 1 G/E Base.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.12","Very High","","","Leak was located from centrifugal filter dome sealing, securing band tightened and this has arrested the leak. Then cleaned the save-all of the oil.","2023-08-21T23:59:35","","Completed","2023-08-02T23:59:35","No","No","No","Internal"]
[null,null,null,31727,65574,"50_Thu Aug 17 2023 23:52:11 GMT+0800","2023-08-01T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","1 No. hot plate in Galley not heating fully","Miscellaneous","MLC Related","Equipment Related","11.13","Low","","","Glass insulated Cable found damaged and same renewed. Hot plate is working satisfactory. ","2023-11-01T23:59:35","","Completed","2023-08-09T23:59:35","No","No","No","Internal"]
[null,null,null,31728,76244,"50_Fri Aug 18 2023 00:05:54 GMT+0800","2023-08-01T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Torn lagging on pipeline on top of COP Platform.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Additional laggings inserted to cover the exposed pipeline.","2023-08-31T23:59:35","","Completed","2023-08-14T23:59:35","No","No","No","Internal"]
[null,null,null,31729,60901,"50_Sat Aug 19 2023 12:03:28 GMT+0800","2023-08-01T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","M2 Mooring winch having hydraulic oil leak near the operating lever.","Deck - Mooring Machinery","Mooring","Equipment Related","9.14","Medium","","","Operating lever box renewed ,leak rectified","2023-08-21T23:59:35","","Completed","2023-08-21T23:59:35","No","No","No","Internal"]
[null,null,null,31730,98954,"50_Sat Aug 19 2023 12:17:33 GMT+0800","2023-08-01T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Heavy weather catwalk wires supports in poor condition.","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.1","High","","","Heavy weather catwalk wires supports checked and bottle screw renewed","2023-09-16T23:59:35","","Completed","2023-08-09T23:59:35","No","No","No","Internal"]
[null,null,null,31731,49257,"0_Sat Aug 19 2023 12:09:29 GMT+0800","2023-08-01T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Oil leak near hydraulic pump in hydraulic valve room.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","6.9","Low","","","Oil leak near hydraulic pump investigated, pipe for external filter observed leaking, same opened new teflon thread seals put and tightened back","2023-09-01T23:59:35","","Completed","2023-08-17T23:59:35","No","No","No","Internal"]
[null,null,null,31732,65194,"0_Sat Aug 19 2023 12:05:54 GMT+0800","2023-08-01T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","CAV 49 Valve of Yellow line port manifold leaking.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.41","Medium","","","CAV 49 Valve of Yellow line port manifold gasket renewed, leak arrested","2023-08-16T23:59:35","","Completed","2023-08-18T23:59:35","No","No","No","Internal"]
[null,null,null,31733,36111,"0_Sat Aug 19 2023 12:04:47 GMT+0800","2023-08-01T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Drain valve of Red line port side manifold leaking.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.41","Medium","","","Drain valve of Red line port side manifold renewed","2023-08-21T23:59:35","","Completed","2023-08-18T23:59:35","No","No","No","Internal"]
[null,null,null,31734,67837,"50_Sat Aug 19 2023 11:50:46 GMT+0800","2023-08-01T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","All ballast tanks manhole butterfly nuts require greasing.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","9.18","Low","","","All ballast tanks manhole butterfly nuts greased","2023-09-01T23:59:35","","Completed","2023-08-11T23:59:35","No","No","No","Internal"]
[null,null,null,31735,83832,"50_Sat Aug 19 2023 11:44:58 GMT+0800","2023-08-01T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Upper deck entrance self closing door not closing fully.","Accommodation","Safety / LSA / FFA","Equipment Related","10.44","Medium","","","Upper deck entrance self closing door rectified","2023-08-21T23:59:35","","Completed","2023-08-21T23:59:35","No","No","No","Internal"]
[null,null,null,31736,14619,"50_Sat Aug 19 2023 11:03:13 GMT+0800","2023-08-01T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Low expansion foam filling line base heavily corroded and wasted.","LSA / FFA","Safety / LSA / FFA","Equipment Related","11.4","Very High","","","Low expansion foam filling line base derusted and pipe thickness checked, found satisfactory, two coats of primer and final coat of top coat applied","2023-11-01T23:59:35","","Completed","2023-08-16T23:59:35","No","No","No","Internal"]
[null,null,null,31737,62609,"50_Sat Aug 19 2023 10:54:59 GMT+0800","2023-08-01T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Spare gratings kept on funnel deck loosely lashed.","Miscellaneous","General Appearance","Inappropriate Procedure","11.5","Medium","","","Spare gratings on funnel deck properly secured with new wire lashings","2023-08-16T23:59:35","","Completed","2023-08-20T23:59:35","No","No","No","Internal"]
[null,null,null,31738,62338,"50_Sat Aug 19 2023 10:29:14 GMT+0800","2023-08-01T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Galley exhaust mesh full of oil and grease.","Accommodation","General Appearance","Inappropriate Procedure","11.13","Low","","","Exhaust mesh opened and cleaned, exhaust fan cleaned and made  free of oil and grease","2023-08-14T23:59:35","","Completed","2023-08-08T23:59:35","No","No","No","Internal"]
[null,null,null,31739,73691,"50_Sat Aug 19 2023 10:16:49 GMT+0800","2023-08-01T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","1 fire hose box on ‘C’ Deck portside lock broken and made fast with rope","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.38","High","","","Fire hose box lock repaired.","2023-08-16T23:59:35","","Completed","2023-08-23T23:59:35","No","No","No","Internal"]
[null,null,null,31741,70744,"50_Wed Aug 16 2023 06:33:37 GMT+0800","2023-08-01T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Water leak from Steam valve behind No 1 Aux boiler.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Water leak found from gland of the water level controller of No.1 Aux boiler. Gland renewed.","2023-08-21T23:59:35","","Completed","2023-08-20T23:59:35","No","No","No","Internal"]
[null,null,null,31742,34860,"50_Sat Aug 19 2023 11:15:24 GMT+0800","2023-08-01T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Chain block for lifting cover of plastic wastes container incorrectly rigged with safety lock of the hooks broken.","Miscellaneous","General Appearance","Equipment Related","10.28","Low","","","Chain block for lifting cover of plastic wastes container correctly rigged and safety lock of the hooks repaired","2023-08-14T23:59:35","","Completed","2023-08-11T23:59:35","No","No","No","Internal"]
[null,null,null,31693,37564,"50_Sun Aug 06 2023 05:06:24 GMT+0800","2023-08-04T23:59:35","Observation","Ship Staff","Ship Staff Insp.","BRIDGE RPM INDICATOR ON STBD SIDE NOT WORKING","Navigation - Others","Navigation","Equipment Related","4.7","High","","","Bridge RPM indicator renewed with new spare.Tried out and working in order.","2023-12-15T23:59:35","","Completed","2024-01-04T23:59:35","No","No","No","Internal"]
[null,null,null,32496,95931,"50_Sat Sep 23 2023 09:12:34 GMT+0800","2023-08-09T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Vessel has a history of accommodation doors falling down during rough / high windy condition. \nIt has happened with outside door of D Deck and C Deck, \nDoors on Upper deck Port and Stbd are also not closing properly with heavy repairs already done by ship staff\nFor permanent solution we have raised Requisition DPEO230157 on 27-Apr-2023 for complete 4 doors and awaiting supply\n","Accommodation","Safety / LSA / FFA","Equipment Related","","","","","awaiting spares\nSpares received and hinges renewed.","2024-02-29T23:59:35","DPEO230157","Completed","2024-02-05T23:59:35","No","No","No","Internal"]
[null,null,null,31721,48793,"50_Mon Aug 21 2023 04:58:00 GMT+0800","2023-08-19T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Control Air Compressor (installed: 05 Feb-2019)  tripping on \"Compressor Element Outlet High Temp. Trip\". When ER ambient temperature goes beyond 43~44 deg C.","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Opened up and cleaned both Oil Cooler and the Air Cooler. Chemical cleaned using ACC 9. Renewed oil, oil filter and Separator Filter. Also cleaned the internal sump of the Separator.","2023-09-19T23:59:35","","Completed","2023-09-09T23:59:35","No","No","No","Internal"]
[null,null,null,32497,30295,"50_Sat Sep 23 2023 09:14:19 GMT+0800","2023-08-23T23:59:35","Observation","Ship Staff","Ship Staff Insp.","STUD ON VAPOUR MANIFOLD IS NOT WELDED TYPE BUT SCREW TO THE MANIFOLD","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.42","Medium","","","VAPOUR MANIFOLD REDUCER TO BE REMOVED AND TAKEN TO E/R WORKSHOP.\nTAG WELDING OF THE CYLINDRICAL STUD TO BE DONE AS PER OPS EMAIL DTD 23 August 2023 \nReducers removed from manifold for Tag welding of cylindrical stud.\nReducers welded with stud and placed back in position.","2023-11-30T23:59:35","","Completed","2023-11-15T23:59:35","No","No","No","Internal"]
[null,null,null,31740,57960,"50_Sat Sep 02 2023 00:33:14 GMT+0800","2023-08-23T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Brake cylinder of M7 winch observed leaking from body while mooring preparation ","Deck - Mooring Machinery","Mooring","Equipment Related","","","","","The said mooring winch brake assembly renewed with spare one on board. Winch brake tested, rendering set at 60%. All found satisfactory","2023-09-01T23:59:35","","Completed","2023-08-23T23:59:35","No","No","No","Internal"]
[null,null,null,32506,11486,"50_Sat Sep 23 2023 09:16:45 GMT+0800","2023-09-08T23:59:35","Observation","Ship Staff","Ship Staff Insp.","ODME Print out faded/Printer defective/ RO DPEO230046 Awaiting supply ","Cargo Mach.","MARPOL Related","Equipment Related","6.13","Low","","","RO RAISED DPEO230046 Awaiting supply \nNew printer installed and found working satisfactorily.","2023-10-31T23:59:35","DPEO230046","Completed","2023-10-26T23:59:35","No","No","No","Internal"]
[null,null,null,32504,31092,"50_Sat Sep 23 2023 08:51:28 GMT+0800","2023-09-12T23:59:35","Observation","Ship Staff","Ship Staff Insp.","SOFA COVERS IN CREW RECREATION ROOM ARE TORN NEED REPLACEMENT","Miscellaneous","MLC Related","Equipment Related","11.13","Low","","","Temporary repairs carried out","2023-12-31T23:59:35","","Completed","2023-10-20T23:59:35","No","No","No","Internal"]
[null,null,null,32508,93286,"50_Sat Sep 23 2023 09:11:10 GMT+0800","2023-09-13T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Observed signs of leakages on the insulation material at multiple locations along the  exhaust piping of Aux engine No.3.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Removed insulation covers and check for tightness of the flange bolts.","2023-10-20T23:59:35","","Completed","2023-09-13T23:59:35","No","No","No","Internal"]
[null,null,null,32503,67126,"50_Sat Sep 23 2023 12:48:17 GMT+0800","2023-09-16T23:59:35","Defect","Ship Staff","Ship Staff Insp.","4 BRIDGE WINDOW GLASS WIPERS FOUND INOPERATIONAL, DURING TESTING.","Navigation - Others","Navigation","Equipment Related","12.10","High","","","TROUBLESHOOTING IN PROGRESS","2023-11-01T23:59:35","","Completed","2023-10-16T23:59:35","No","No","No","Internal"]
[null,null,null,32507,51423,"50_Sat Sep 23 2023 09:20:33 GMT+0800","2023-09-18T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","Sludge Pump CON ROD failure, Pump totally inoperable.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Dismantled the pump and fabricated onboard CON ROD, still working in good condition.  Vessel shall change with new spare during quarterly check-up of the pump.","2023-10-14T23:59:35","DPEO230137 - URGENT SPARE CON ROD  FOR SLUDGE PUMP","Completed","2023-10-23T23:59:35","No","No","No","Internal"]
[null,null,null,32502,75299,"50_Sat Sep 23 2023 12:42:34 GMT+0800","2023-09-20T23:59:35","Defect","Ship Staff","Ship Staff Insp.","SAT-C -JUE 87 SHOWING ERROR - DTE MAIN DRIVE UNREADABLE, AND ALSO \nIT IS NOT ABLE TO DETECT THE PRINTER .","Navigation - GMDSS & Communication","Navigation","Equipment Related","4.23","High","","","PRINTER CHECKED WITH OTHER SAT-C, IT IS OPERATIONAL, SUSPECTING ISSUES WITH THE SAT-C TERMINAL ONLY, FLASH ROM MIGHT BE TROUBLED .TROUBLESHOOTING BY SHIP'S STAFF IN PROGRESS/SORTED OUT THE ISSUE WITH MAKERS GUIDED ASSISTANCE","2023-11-01T23:59:35","","Completed","2023-09-27T23:59:35","No","No","No","Internal"]
[null,null,null,32499,30049,"50_Wed Oct 18 2023 15:54:58 GMT+0800","2023-10-13T23:59:35","Observation","Ship Staff","Ship Staff Insp.","VRCS pump no.1 , start switch Light not coming on. Require to change the whole power switch","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","Repair the start switch with indicator light and same worked for some time showing the light indication. But indication again has gone defective. To raise new RO for spare start push button switch with light indication.\nStart push button switch replaced with the spare onboard. Working satisfactorily.\n","2024-02-29T23:59:35","","Completed","2024-02-16T23:59:35","No","No","No","Internal"]
[null,null,null,32498,72760,"50_Tue Oct 17 2023 22:49:30 GMT+0800","2023-10-17T23:59:35","Observation","Ship Staff","Ship Staff Insp.","All Fwd, aft and Midship drafts not coming on Emerson computer screen","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","After troubleshooting onboard office has been informed for further assistance.\nShore technician attended the vessel on 19Th October 2023 at Singapore and analyzed that there is software issue which will be solved by manufacturer itself. Vessel awaiting further action.\n\nShore technician attended in Singapore and now Emerson displaying the drafts","2024-04-09T23:59:35","","Completed","2024-04-08T23:59:35","No","No","No","Internal"]
[null,null,null,34714,14617,"50_Tue Mar 26 2024 16:58:34 GMT+0800","2023-10-18T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","IT WAS OBSERVED THAT PCB OF TELEPHONE EXCHANGE UNIT WAS BLOWN OFF. RESULTING IN INTERNAL COMMUNICATION FAILURE.\n","Accommodation","Eng. / Strg. Comp.","Equipment Related","","","","","SHORE TECHNICIAN ATTENDED AND COMPLETED THE JOB.","2024-04-09T23:59:35","DPEO245021","Completed","2024-04-10T23:59:35","No","No","No","Internal"]
[null,null,null,32505,59672,"50_Tue Oct 24 2023 16:07:53 GMT+0800","2023-10-21T23:59:35","Defect","Ship Staff","Ship Staff Insp.","IT WAS OBSERVED THAT FORWARD VOID SPACE HIGH LEVEL ALARM SHOWING FALSE ALARM.","Hull & Tanks","Structural Condn. / WT integrity ","Equipment Related","2.9","Medium","","","INSPECTION OF THE VOID SPACE CARRIED OUT AND SAME FOUND TO BE EMPTY. TROUBLE SHOOTING IN PROGRESS.\nCLEANING OF THE FLOAT AND ASSISTED ASSEMBLY CARRIED OUT. NO ALARMS OBSERVED.\nHIGH LEVEL ALRAM TRIED OUT AND RESET. \nMONITORING OF THE SYSTEM WILL BE IN PLACE.","2023-11-20T23:59:35","","Completed","2023-10-26T23:59:35","No","No","No","Internal"]
[null,null,null,32509,96518,"50_Fri Nov 03 2023 10:48:28 GMT+0800","2023-11-01T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","During pump room routine round it was found that deck seal overboard drain line holed.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","6.4","High","","","Wasted line fabricated, Fixed back and tried out.","2023-11-05T23:59:35","","Completed","2023-11-02T23:59:35","No","No","No","Internal"]
[null,null,null,32501,85339,"50_Wed Nov 15 2023 06:35:02 GMT+0800","2023-11-08T23:59:35","Other","Owner / Marine / Tech. Suptd.","Engineering Audit","SAFETY CIRCULAR/S-009-2023 - Safety Notice issued for CO2 system cylinders manufactured by NK Co. LTD\n1. . All vessels fitted with NK Co. Ltd CO2 Fixed Fire-extinguishing System installed prior 2016, must take note that the bursting disc material is changed from Copper to Nickle. ","LSA / FFA","Safety / LSA / FFA","Industry Issue","5.35","Medium","","","1. Record in DDRL and update vessel Technical Fleet regarding this pending job.\n2. Carried-out an external check of the fixed CO2 system and found that bursting disc of all CO2 cylinders are intact. \n3. Carry out a Risk Assessment because vessel has a fixed CO2 system, which is known to have a defective bursting disc.\n4. Save and replaced on board the attached User Manual, which is provided by the Maker.\n5.Defect recorded in REFMAN as the job can be carried out in dry dock.","2024-04-09T23:59:35","","Completed","2024-03-23T23:59:35","No","No","No","Internal"]
[null,null,null,33385,74411,"50_Thu Nov 30 2023 14:37:37 GMT+0800","2023-11-27T23:59:35","Observation","Ship Staff","Ship Staff Insp.","During routine inspection it was observed that No.4 Foam monitor valve stuck in closed position. ","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.38","High","","","No.4 foam monitor valve freed and greased.","2023-12-01T23:59:35","","Completed","2023-11-30T23:59:35","No","No","No","Internal"]
[null,null,null,33388,60750,"50_Tue Dec 05 2023 16:04:08 GMT+0800","2023-11-30T23:59:35","Observation","Ship Staff","Ship Staff Insp.","During routine wet round on deck it was observed that marking on life buoys were faded.","LSA / FFA","Safety / LSA / FFA","Knowledge Based","5.31","High","","","Lifebuoys marking were stenciled.","2023-12-05T23:59:35","","Completed","2023-12-02T23:59:35","No","No","No","Internal"]
[null,null,null,33386,35966,"50_Tue Dec 05 2023 15:43:50 GMT+0800","2023-12-04T23:59:35","Defect","Ship Staff","Ship Staff Insp.","DURING CARGO LINE PRESSURE TEST VESSEL FOUND NO 4 MANIFOLD VALVE STBD SIDE LEAKING. SUSPECT SEAT RING DAMAGED.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.8","Medium","","","REMOVAL OF VALVE TO BE CARRIED OUT. \nRENEWAL OF SEAT RING TO BE CARRIED OUT.\nPO DPEO230345 RAISED, VESSEL AWAITING SPARES.\nNO4 MANIFOLD STBD SIDE SEATRING RENEWED.","2024-01-10T23:59:35","DPEO230345","Completed","2023-12-27T23:59:35","No","No","No","Internal"]
[null,null,null,28199,59440,"0_Tue Dec 27 2022 05:46:33 GMT+0800","2023-12-15T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Securing pins, for lifebuoys rusted","LSA / FFA","Safety / LSA / FFA","Behaviour Based","5.31","High","","","Derusting and painting of lifebouys securing pin carried out.","2023-03-14T23:59:35","","Completed","2022-12-18T23:59:35","No","No","No","Internal"]
[null,null,null,33387,12593,"50_Sun Jan 07 2024 00:06:58 GMT+0800","2024-01-02T23:59:35","Observation","Ship Staff","Ship Staff Insp.","During safety round it was observed that Port and Stbd MOB lifebouy cradle foudn to be rusted","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.31","High","","","Port and Stbd MOB lifebouy cradle derusted and painted.","2024-01-05T23:59:35","","Completed","2024-01-05T23:59:35","No","No","No","Internal"]
[null,null,null,33814,18102,"50_Sat Feb 03 2024 06:20:42 GMT+0800","2024-01-10T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Knocking sound coming from the ME exhuast valve of unit no:1","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Ship staff has carried out checks per the maker and plan to carry out checks on the actuator pressure limiting valve at the next opportunity.","2024-06-30T23:59:35","","Completed","2024-05-17T23:59:35","No","No","No","Internal"]
[null,null,null,34454,45136,"50_Fri Feb 23 2024 13:48:26 GMT+0800","2024-01-10T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Slop S overfill alarm knob found to be frozen ","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","Slop S overfill alarm knob freed and tried out. Found working satisfactorily.","2024-01-20T23:59:35","","Completed","2024-01-17T23:59:35","No","No","No","Internal"]
[null,null,null,33809,63391,"50_Sat Feb 03 2024 06:23:01 GMT+0800","2024-01-23T23:59:35","Defect","Ship Staff","Ship Staff Insp.","AE NO:1 AND 2 T/C RPM sensors showing faulty indication","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Ship staff checked both AE turbocharger rpm sensors connection , found little loose , same tightened properly , AE 1 & 2 tried out , found T/C rpm sensors showing correct reading.","2024-02-29T23:59:35","","Completed","2024-02-06T23:59:35","No","No","No","Internal"]
[null,null,null,34722,25164,"50_Tue Mar 26 2024 17:03:27 GMT+0800","2024-01-24T23:59:35","Observation","Ship Staff","Ship Staff Insp.","HMI Operating panel of AHU and AC plant is faded out.","Accommodation","Eng. / Strg. Comp.","Equipment Related","","","","","HMI PANEL RENEWED BY TECHNICANS AND BOTH AIR COMPRESSORS TRIED OUT IN AUTO.FOUND WORKING IN ORDER.","2024-12-15T23:59:35","DPEO240018","Completed","2024-12-01T23:59:35","No","No","Yes","Internal"]
[null,null,null,33813,54280,"50_Sat Feb 03 2024 06:44:12 GMT+0800","2024-01-26T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Suction valve and discharge non valve for emergency fire pump found passing","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","","","","","discharge valve renewed.","2024-09-15T23:59:35","","Completed","2024-09-05T23:59:35","No","No","Yes","Internal","Mention RO number"]
[null,null,null,33816,41086,"50_Sat Feb 03 2024 02:13:28 GMT+0800","2024-01-30T23:59:35","Observation","Ship Staff","Ship Staff Insp.","EGCS ME Bypass valve actuator found with slight air leakage","","Eng. / Strg. Comp.","Equipment Related","","","","","EGCS ME Bypass valve actuator repaired and put in service ","2024-07-15T23:59:35","","Completed","2024-07-11T23:59:35","No","No","No","Internal"]
[null,null,null,33807,63697,"50_Sat Feb 03 2024 02:05:20 GMT+0800","2024-01-31T23:59:35","Defect","Ship Staff","Ship Staff Insp.","ME unit no:3,5,6 Local exhaust gas thermometers not working","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Unit no:3,5,6 exhaust gas pockets renewed spare ones.Exhaust gas thermometers showing temperature in order.","2024-03-29T23:59:35","","Completed","2024-03-25T23:59:35","No","No","No","Internal"]
[null,null,null,33808,17575,"50_Sat Feb 03 2024 02:08:27 GMT+0800","2024-01-31T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Boiler water circulating no:2 coupling broken","E/R - Pumps","Eng. / Strg. Comp.","","","","","","New cooler and its connections were installed for mechanical seal cooling. Spare new coupling is recieved by the vessel. Ship staff will plan to renew the complete coupling  at the next possible opportunity.","2024-06-30T23:59:35","","Completed","2024-05-23T23:59:35","No","No","No","Internal"]
[null,null,null,34450,92034,"50_Sat Feb 24 2024 17:15:05 GMT+0800","2024-02-07T23:59:35","Observation","Ship Staff","Ship Staff Insp.","ME and DG main and bypass dampers to be inspected","E/R - Main Engine,E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","ME AND DG BYPASS DUMPER CHECK OPERATION DURING CHANGE OVER AND FOUND ALL WORKING SATISFACTORY","2024-07-15T23:59:35","","Completed","2024-07-10T23:59:35","No","No","No","Internal"]
[null,null,null,34692,92165,"50_Sun Mar 03 2024 14:09:51 GMT+0800","2024-02-12T23:59:35","Observation","Ship Staff","Ship Staff Insp.","It was found that M5 winch is moving/reacting very slowly even after the hydraulic system for mooring has been started","Deck - Mooring Machinery","Mooring","Equipment Related","","","","","To check and investigate\n\nM5 winch adjusted and now working in order","2024-05-11T23:59:35","","Completed","2024-02-21T23:59:35","No","No","No","Internal"]
[null,null,null,34718,65949,"50_Tue Mar 26 2024 17:29:56 GMT+0800","2024-02-15T23:59:35","Defect","Ship Staff","Ship Staff Insp.","STBD side rudder angle indicator fully in operational/Port side rudder Y angle indicator only dimmer switch in operational","Elect. Mach. & Equip.","Navigation","Equipment Related","","","","","DUPLICATED ENTRY roubleshooting carried out and RO DPEO240085 placed for the same","2024-08-30T23:59:35","DPEO240085","Completed","2024-08-01T23:59:35","No","No","No","Internal"]
[null,null,null,34693,91345,"50_Sun Mar 03 2024 13:39:18 GMT+0800","2024-02-19T23:59:35","Observation","Ship Staff","Ship Staff Insp.","RPM indicator on bridge wing found to be stuck at a particular RPM","Navigation - Others","Navigation","Equipment Related","","","","","Trouble shooting and repair for RPM indicator carried out and now working in order","2024-05-15T23:59:35","","Completed","2024-02-27T23:59:35","No","No","No","Internal"]
[null,null,null,34694,73099,"50_Sun Mar 03 2024 13:36:30 GMT+0800","2024-02-19T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Buzzer for SAAB Radar found not be loud for any alarms","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","Buzzer sound increased and now buzzer working fine","2024-05-15T23:59:35","","Completed","2024-02-26T23:59:35","No","No","No","Internal"]
[null,null,null,34453,71458,"50_Sat Feb 24 2024 17:10:54 GMT+0800","2024-02-20T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Air compressor No:3 cylinder cover wasted.","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related","","","","","Air compressor no3 HP piston found broken and liner damaged.On further inspection it was found that the cylinder cover HP valve seat collar is wasted away leading to breaking of HP discharge valve and other damages.HP piston and liner renewed.RO placed for a new cylinder cover.( DPEO 240056)","2024-06-30T23:59:35","DPEO240056","Completed","2024-05-27T23:59:35","No","No","No","Internal"]
[null,null,null,34455,96243,"50_Sat Mar 02 2024 12:39:33 GMT+0800","2024-02-26T23:59:35","Observation","Ship Staff","Ship Staff Insp.","PV breaker sight glass not in good condition and frame found to be corroded.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.28","Medium","","","Sight glass renewed and new frame and brackets made for PV breaker","2024-03-05T23:59:35","","Completed","2024-03-01T23:59:35","No","No","No","Internal"]
[null,null,null,34456,78389,"50_Sat Mar 02 2024 12:41:53 GMT+0800","2024-02-26T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Deck seal overboard pipe found to be rusted and pin hole found on the overboard line","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.23","Medium","","","Deck seal overboard line renewed with new one","2024-03-06T23:59:35","","Completed","2024-03-01T23:59:35","No","No","No","Internal"]
[null,null,null,34452,79108,"50_Sat Mar 02 2024 20:27:17 GMT+0800","2024-02-28T23:59:35","Observation","Ship Staff","Ship Staff Insp.","ME T/C No:1 is surging at 9500RPM","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Ship staff suspects that the Nozzle ring is fouled with carbon deposits.The turbocharger gas inlet temperature of both turbochragers are high.As per correspondence with office,nozzle ring will be cleaned at singapore (march 2023)","2024-04-09T23:59:35","DPEO245019","Completed","2024-04-10T23:59:35","No","No","No","Internal"]
[null,null,null,34717,29085,"50_Tue Mar 26 2024 17:31:52 GMT+0800","2024-02-28T23:59:35","Defect","Ship Staff","Ship Staff Insp.","COP no:1 mechanical seal overflow high level alarm float not working","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","Alarms tested, found in working condition.","2024-10-30T23:59:35","DPEO240086","Completed","2024-09-30T23:59:35","No","No","Yes","Internal"]
[null,null,null,34723,22145,"50_Tue Mar 26 2024 17:26:03 GMT+0800","2024-03-13T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Cargo tank monitor alarm buzzer sound is very low","Elect. Mach. & Equip.","Cargo / Ballast Systems","Equipment Related","","","","","Vessel will plan to install seperate buzzer of 24V.\nNew buzzer and connection carried out. Working satisfactorily.","2024-04-09T23:59:35","","Completed","2024-04-08T23:59:35","No","No","No","Internal"]
[null,null,null,34719,94391,"50_Tue Mar 26 2024 17:35:21 GMT+0800","2024-03-18T23:59:35","Defect","Ship Staff","Ship Staff Insp.","5C SAAB radar communication failure","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","Troubleshooting carried out and found TGU unit faulty.RO placed for the same.\n\nNew TGE unit fitted by shore technician at Singapore","2024-04-09T23:59:35","DPEO245020","Completed","2024-04-08T23:59:35","No","No","No","Internal"]
[null,null,null,34724,38294,"50_Tue Mar 26 2024 17:06:39 GMT+0800","2024-03-22T23:59:35","Defect","Ship Staff","Ship Staff Insp.","The bulb of the telephone call in the alarm signalling of the workshop was found not working","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","The bulb renewed with a spare one.All the indications in the alarm signalling unit are working.","2024-03-25T23:59:35","","Completed","2024-03-25T23:59:35","No","No","No","Internal"]
[null,null,null,34725,99230,"50_Tue Mar 26 2024 17:21:08 GMT+0800","2024-03-23T23:59:35","Observation","Ship Staff","Ship Staff Insp.","The cop 1,2,3 guards were not found effective in preventing a hazard","","Eng. / Strg. Comp.","Equipment Related","","","","","New guards covering the entire exposed are of the COP turbine coupling fabricated and fitted.","2024-03-25T23:59:35","","Completed","2024-03-24T23:59:35","No","No","No","Internal"]
[null,null,null,34726,68813,"50_Tue Mar 26 2024 17:22:49 GMT+0800","2024-03-23T23:59:35","Observation","Ship Staff","Ship Staff Insp.","The emergency lighting in the Midship locker above the firemans outfit not marked with emergency marking","Elect. Mach. & Equip.","Emgcy. Systems","Equipment Related","","","","","Emergency marking carried out for the emergency lighting in Midship locker.","2024-03-24T23:59:35","","Completed","2024-03-25T23:59:35","No","No","No","Internal"]
[null,null,null,35093,10753,"50_Mon Apr 22 2024 12:42:04 GMT+0800","2024-04-10T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Ship Staff Insp.","Hydraulic oil leaks noted at M2 and M3 Winches","Deck - Mooring Machinery","Mooring","Equipment Related","","","","","To renew the oil seal and test\n\nBlock renewed for M3 winch and O-rings renewed for M2 winch. Tested and found free of leaks.","2024-07-10T23:59:35","","Completed","2024-05-24T23:59:35","No","No","No","Internal"]
[null,null,null,35094,28989,"50_Mon Apr 22 2024 12:44:22 GMT+0800","2024-04-10T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Ship Staff Insp.","Both lifeboat hooks require de-rusting and greasing/painting. The markings on the hooks have faded","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","De-rusting , painting and greasing of Life boat hooks both P & S side is completed. Markings renewed.","2024-10-10T23:59:35","","Completed","2024-08-15T23:59:35","No","No","No","Internal"]
[null,null,null,35098,67070,"50_Mon Apr 22 2024 12:43:20 GMT+0800","2024-04-10T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Oil leakage noted in Boxes No. 2 and 3 of Hydraulic Valve Solenoids","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","Oil to be cleaned .\n\nOil cleaned in all the hydraulic boxes","2024-07-10T23:59:35","","Completed","2024-04-22T23:59:35","No","No","No","Internal"]
[null,null,null,35989,78507,"50_Wed May 15 2024 09:34:27 GMT+0800","2024-04-15T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Aux engine no 2 having leak from leakage pot.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","leakage rectified.","2024-06-15T23:59:35","","Completed","2024-06-18T23:59:35","No","No","No","Internal"]
[null,null,null,35990,16114,"50_Wed May 15 2024 09:43:19 GMT+0800","2024-04-15T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Lagging of exhaust pipe passing between engine casing and scrubber room is damage.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","Lagging repair carried out.","2024-10-31T23:59:35","","Completed","2024-10-22T23:59:35","No","No","No","Internal"]
[null,null,null,35993,54440,"50_Wed May 15 2024 09:37:10 GMT+0800","2024-04-15T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Jacket water 3 way valve of ME having leak from gland.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","Packing  renewed.","2024-06-26T23:59:35","","Completed","2024-06-26T23:59:35","No","No","No","Internal"]
[null,null,null,36000,74272,"50_Wed May 15 2024 07:18:33 GMT+0800","2024-04-15T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Both boiler feed water valves leaking from gland.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","Gland to be tighthened.","2024-06-30T23:59:35","","Completed","2024-05-20T23:59:35","No","No","No","Internal"]
[null,null,null,36001,19224,"50_Wed May 15 2024 07:12:47 GMT+0800","2024-04-15T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Aft no. 2 deck hydraulic pump coupling missing .","Deck - Mooring Machinery","Mooring","Equipment Related","","","","","Spider coupling to be fitted.","2024-06-30T23:59:35","","Completed","2024-05-30T23:59:35","No","No","No","Internal"]
[null,null,null,36002,70319,"50_Wed May 15 2024 07:15:20 GMT+0800","2024-04-15T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","No. 1 and 2 DG centrifugal filter having leak.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Orings to be renewed.","2024-06-15T23:59:35","","Completed","2024-05-31T23:59:35","No","No","No","Internal"]
[null,null,null,36003,50967,"50_Wed May 15 2024 07:46:02 GMT+0800","2024-04-15T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Aux engine no 3 FO supply pump leaking from mechanical seal.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Mechanical seal to be replaced.","2024-06-15T23:59:35","","Completed","2024-05-31T23:59:35","No","No","No","Internal"]
[null,null,null,36005,89455,"50_Wed May 15 2024 07:22:38 GMT+0800","2024-04-15T23:59:35","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Poster to display near all tanks,  no gagging of tha gauge glass spring valves.","Miscellaneous","Eng. / Strg. Comp.","External Factors","","","","","Poster to display","2024-06-30T23:59:35","","Completed","2024-05-18T23:59:35","No","No","No","Internal"]
[null,null,null,36007,68425,"50_Wed May 15 2024 07:35:56 GMT+0800","2024-04-15T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","3 hot plates are not getting hot enough.","Miscellaneous","MLC Related","Equipment Related","","","","","Hot plates to be renewed.","2024-06-30T23:59:35","","Completed","2024-05-24T23:59:35","No","No","No","Internal"]
[null,null,null,36008,43523,"50_Wed May 15 2024 07:43:30 GMT+0800","2024-04-15T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Oil leakage to near me air cooler","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","Bolts to tight.","2024-06-30T23:59:35","","Completed","2024-05-20T23:59:35","No","No","No","Internal"]
[null,null,null,36009,60593,"50_Wed May 15 2024 08:48:11 GMT+0800","2024-04-15T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Aux boiler lagging is missing","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related,External Factors","","","","","Lagging to be fitted back","2024-06-30T23:59:35","","Completed","2024-05-17T23:59:35","No","No","No","Internal"]
[null,null,null,36010,75147,"50_Wed May 15 2024 07:29:56 GMT+0800","2024-04-15T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","All steps near ME cylinder head are not secure properly.","Miscellaneous","Eng. / Strg. Comp.","External Factors","","","","","Steps to be fitted with with angle bars.","2024-06-30T23:59:35","","Completed","2024-05-23T23:59:35","No","No","No","Internal"]
[null,null,null,35096,35274,"50_Wed May 01 2024 20:50:32 GMT+0800","2024-05-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","MAC NO 3 INOPERATIONAL","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related","","","","","CYLINDER HEAD, PISTON RENEWED WITH NEW SPARE.","2024-07-01T23:59:35","","Completed","2024-05-24T23:59:35","No","No","Yes","Internal"]
[null,null,null,35097,86743,"50_Wed May 01 2024 20:31:19 GMT+0800","2024-05-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","HFO Purifier no. 2 inoperational,","E/R - Purifier","Eng. / Strg. Comp.","Equipment Related","","","",""," Checks and trouble shooting as per maker guidlines carried out but still problem persist.","2024-06-15T23:59:35","","Completed","2024-05-17T23:59:35","No","No","No","Internal"]
[null,null,null,35099,36345,"50_Sat May 11 2024 16:47:48 GMT+0800","2024-05-06T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Dump valves for port and starboard Slop tanks found to be very tight for operation.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","Dump valves to be greased and freed and tried for operation.\n\nDump valves greased and freed. Working satisfactorily.","2024-05-11T23:59:35","","Completed","2024-05-10T23:59:35","No","No","No","Internal"]
[null,null,null,36329,85643,"50_Sat Jun 15 2024 03:06:28 GMT+0800","2024-05-15T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Main isolation valve for M6 winch found to leaking.","Deck - Mooring Machinery","Mooring","Equipment Related","","","","","DPEO240133 - SHUT OFF VALVE FOR AFT MOORING WINCH  , NEW SHUT OFF VALVE RECIEVED ON 01-12-2024.SAME WILL BE FITTED AT SEA\nnew received valve fitted no leak observed","2024-12-15T23:59:35","DPEO240133 - SHUT OFF VALVE FOR AFT MOORING WINCH ","Completed","2024-12-05T23:59:35","No","No","No","Internal"]
[null,null,null,35991,31853,"50_Fri May 31 2024 09:35:15 GMT+0800","2024-05-30T23:59:35","Defect","Ship Staff","Ship Staff Insp.","AFT HYDRAULIC POWER PACK FOUND WATER CONTENT IN OIL","Deck - Mooring Machinery","Eng. / Strg. Comp.","Equipment Related","","","","","OLD LO COOLER REMOVED AND INSTALLED NEW LO COOLER DUE TO SOME TUBES ARE LEAKAGE AND SOME ARE PLUGS ,   CONTAMINATED  OIL DRAIN  INCLUDING THE LINE \nAND CLEANED PROPERLY INSIDE THE TANK AND PUT NEW OIL.","2024-07-15T23:59:35","","Completed","2024-05-30T23:59:35","No","No","No","Internal"]
[null,null,null,35992,64998,"50_Fri May 31 2024 09:46:41 GMT+0800","2024-05-30T23:59:35","Defect","Ship Staff","Ship Staff Insp.","FWG SECTION OF SW INLET  PIPE IS HAVING COLD WORK","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","",""," PIPE RENEWED","2024-06-15T23:59:35","","Completed","2024-06-26T23:59:35","No","No","No","Internal"]
[null,null,null,35994,71829,"50_Fri May 31 2024 09:42:46 GMT+0800","2024-05-30T23:59:35","Defect","Ship Staff","Ship Staff Insp.","HARBOR SW PUMP FOUND SEIZED","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","","","","","Harbour cooling sea water puump coupling eased up,pump found rotating smoothly.Pump started and found suction,discharge pressure and amperage satisfactory.","2024-09-30T23:59:35","","Completed","2024-09-05T23:59:35","No","No","No","Internal","No RO number mentioned."]
[null,null,null,35996,30446,"50_Fri May 31 2024 09:49:39 GMT+0800","2024-05-30T23:59:35","Defect","Ship Staff","Ship Staff Insp.","MAIN ENGINE JACKET WATER CONTROLER IS LEAKING","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","INSPECTED AND GLAND PACKING RENEWED","2024-06-15T23:59:35","","Completed","2024-06-26T23:59:35","No","No","No","Internal"]
[null,null,null,35998,85352,"50_Sat Jun 01 2024 15:12:55 GMT+0800","2024-05-30T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Steering gear room vent mushroom ladder bent","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","Job completed.","2024-09-30T23:59:35","","Completed","2024-08-19T23:59:35","No","No","No","Internal","Update status."]
[null,null,null,35999,18473,"50_Fri May 31 2024 09:55:05 GMT+0800","2024-05-30T23:59:35","Defect","Ship Staff","Ship Staff Insp.","MAC NO 3 SOFT STARTER IS HAVING LOW INSULATION","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related","","","","","TROUBLE SHOOT CARRIED-OUT AND FOUND HAS NO PROBLEM  ON THE SOFT STARTER. WIRE INTERCONNECTION CHECK AND CORRECTLY CHANGE AND COMPRESSOR TRIED-OUT  FINE WORKING SATISFACTORY. INSULATION WAS COMING FROM LO PRESSURE SWITCH ","2024-07-30T23:59:35","DPEO240148","Completed","2024-08-01T23:59:35","No","No","No","Internal"]
[null,null,null,36004,61685,"50_Fri May 31 2024 09:39:56 GMT+0800","2024-05-30T23:59:35","Defect","Ship Staff","Ship Staff Insp.","PUMPROOM  FAN NO 2 STUFFING BOX TEMP IS ON THE HIGHER SIDE","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","STUFFING BOX BEARING RENEWED , shaft also changed ","2024-06-15T23:59:35","","Completed","2024-06-02T23:59:35","No","No","No","Internal"]
[null,null,null,36006,41514,"50_Fri May 31 2024 09:31:39 GMT+0800","2024-05-30T23:59:35","Defect","Ship Staff","Ship Staff Insp.","AFT HYDRAULIC COOLER FOUND TO BE LEAKING","Deck - Mooring Machinery","Eng. / Strg. Comp.","Equipment Related","","","","","TO BE REPLACED WITH NEW SPARE.","2024-06-15T23:59:35","AFT HYDRAULIC COOLER TO BE REPLACED WITH NEW SPARE","Completed","2024-05-30T23:59:35","No","No","No","Internal"]
[null,null,null,34715,77178,"50_Tue Mar 26 2024 17:00:56 GMT+0800","2024-06-09T23:59:35","Defect","Ship Staff","Ship Staff Insp.","LT Coolers fwd and aft strainers found partially damaged","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Filters temporarily repaired. Office informed and drawings of the filter forwarded to office for new strainer.( DPEO245010).New strainer recieved on 01-12-2024.LT cooler fwd fitted with new strainer.RO to be placed for aft strainer as only one piece was recieved.","2024-12-15T23:59:35","DPEO245010-FABRICATION OF LT COOLER STRAINER","Completed","2024-12-02T23:59:35","No","No","Yes","Internal"]
[null,null,null,37786,88075,"50_Sun Sep 29 2024 02:16:15 GMT+0800","2024-06-14T23:59:35","Non Conformity","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Port side hose handling crane hook observed without safety lock.  Not  permitted to use crane for lifting work.","Cargo Mach.","Safety / LSA / FFA","Equipment Related","","","","","Port side hose handling crane hook lock renewed.","2024-11-30T23:59:35","","Completed","2024-06-14T23:59:35","No","No","No","Internal"]
[null,null,null,37783,90566,"50_Sun Sep 29 2024 02:08:47 GMT+0800","2024-06-15T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Monkey island air supply valve and line to whistle requires de-rust and paint","Deck - Pipe / Fittings","General Appearance","Equipment Related","","","","","De-rusting and painting of Air supply line is completed.","2024-10-31T23:59:35","","Completed","2024-08-08T23:59:35","No","No","No","Internal"]
[null,null,null,37784,12624,"50_Sun Sep 29 2024 02:12:27 GMT+0800","2024-06-15T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Bridge wing supports have scattered rust and corrosion to de-rust and paint.","Accommodation","General Appearance","Equipment Related","","","","","Bridge wing supports  de-rust and painting completed.","2024-11-30T23:59:35","","Completed","2024-08-17T23:59:35","No","No","No","Internal"]
[null,null,null,37785,39632,"50_Sun Sep 29 2024 02:18:43 GMT+0800","2024-06-15T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Port side lifeboat embarkation ladder canvas cover to renew.","LSA / FFA","General Appearance","Equipment Related","","","","","Port side lifeboat embarkation ladder canvas cover to renewed.","2024-11-30T23:59:35","","Completed","2024-07-09T23:59:35","No","No","No","Internal"]
[null,null,null,37787,69798,"50_Sun Sep 29 2024 02:21:41 GMT+0800","2024-06-15T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Port HFO tank ullage/ sampling pipe to de-rust and paint","Hull & Tanks,Deck - Pipe / Fittings","General Appearance","Equipment Related","","","","","Port HFO tank ullage/ sampling pipe  de-rusting and painting completed.","2024-11-30T23:59:35","","Completed","2024-07-13T23:59:35","No","No","No","Internal"]
[null,null,null,37788,21969,"50_Sun Sep 29 2024 02:24:58 GMT+0800","2024-06-15T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","HFO tank entrance hatch  to de-rust and paint.","Deck - Pipe / Fittings","General Appearance","Equipment Related","","","","","HFO tank entrance hatch de-rusting and painting completed.","2024-11-30T23:59:35","","Completed","2024-07-13T23:59:35","No","No","No","Internal"]
[null,null,null,37789,13346,"50_Sun Sep 29 2024 02:38:20 GMT+0800","2024-06-15T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Marpol IOPP and sewage discharge connection and save all to de-rust and paint.","Deck - Pipe / Fittings","General Appearance","Equipment Related","","","","","Marpol IOPP and sewage discharge connection and save all tray de-rusting and painting completed.","2024-11-30T23:59:35","","Completed","2024-09-15T23:59:35","No","No","No","Internal"]
[null,null,null,37790,21930,"50_Sun Sep 29 2024 02:49:10 GMT+0800","2024-06-15T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Numerous manhole on deck require power tooling, descale and paint.","Hull & Tanks","General Appearance","Equipment Related","","","","","Deck manholes descaling and painting completed.","2024-11-30T23:59:35","","Completed","2024-07-26T23:59:35","No","No","No","Internal"]
[null,null,null,37791,26822,"50_Sun Sep 29 2024 02:52:44 GMT+0800","2024-06-15T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","HFO tank save all and air pipe to de-rust and paint.","Deck - Pipe / Fittings","General Appearance","Equipment Related","","","","","HFO tank save all and air pipe de-rusting and painting completed.","2024-11-30T23:59:35","","Completed","2024-09-15T23:59:35","No","No","No","Internal"]
[null,null,null,37792,78355,"50_Sun Sep 29 2024 03:06:49 GMT+0800","2024-06-15T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Deck air line valve on deck near 3 stbd COT to maintain.","Deck - Pipe / Fittings","ISM Related","Equipment Related","","","","","Deck air line valve on deck near 3 stbd COT maintenance carried out.","2024-11-30T23:59:35","","Completed","2024-08-09T23:59:35","No","No","No","Internal"]
[null,null,null,37793,73718,"50_Sun Sep 29 2024 03:42:28 GMT+0800","2024-06-15T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","PV Breaker for 3C Heavy WX Ballast to renew Gauge glass holder and flanges to derust","Cargo Mach.","ISM Related","Equipment Related","","","","","PV Breaker for 3C Heavy WX Ballast  renewed Gauge glass holder and flanges derusted","2024-11-30T23:59:35","","Completed","2024-07-20T23:59:35","No","No","No","Internal"]
[null,null,null,37794,19150,"50_Sun Sep 29 2024 03:45:36 GMT+0800","2024-06-15T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Securing U-bolts on deck IG line Corroded in most places. To descale and paint","Deck - Pipe / Fittings","ISM Related","Equipment Related","","","","","Securing U-bolts on deck IG line descaling and painting completed","2024-11-30T23:59:35","","Completed","2024-08-09T23:59:35","No","No","No","Internal"]
[null,null,null,37795,51507,"50_Sun Sep 29 2024 03:47:43 GMT+0800","2024-06-15T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Port slop tank steam heating coil band to de-rust and paint with heat resistant coating","Deck - Pipe / Fittings","ISM Related","Equipment Related","","","","","Port slop tank steam heating coil band to de-rusted and painted with heat resistant coating","2024-10-31T23:59:35","","Completed","2024-08-10T23:59:35","No","No","No","Internal"]
[null,null,null,37796,89317,"50_Sun Sep 29 2024 03:54:03 GMT+0800","2024-06-15T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Numerous sections of ship's side railings on deck corroded.","Deck - Pipe / Fittings","ISM Related","Equipment Related","","","","","ship's side railings Derusted and painted","2024-10-31T23:59:35","","Completed","2024-07-24T23:59:35","No","No","No","Internal"]
[null,null,null,37797,85525,"50_Sun Sep 29 2024 03:50:10 GMT+0800","2024-06-15T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","HFO save all on STBD side on poop deck to derust , Clean and paint","Deck - Pipe / Fittings","ISM Related","Equipment Related","","","","","HFO save all on STBD side on poop deck to derusted , Cleaned and painted","2024-11-30T23:59:35","","Completed","2024-09-15T23:59:35","No","No","No","Internal"]
[null,null,null,37798,77835,"50_Sun Sep 29 2024 03:55:49 GMT+0800","2024-06-15T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Several ballast tank air pipes require maintenance","Deck - Pipe / Fittings","ISM Related","Equipment Related","","","",""," Ballast tank air pipes maintenance carried out","2024-11-30T23:59:35","","Completed","2024-07-27T23:59:35","No","No","No","Internal"]
[null,null,null,37799,41159,"50_Sun Sep 29 2024 03:57:31 GMT+0800","2024-06-15T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Sections of pipelines on deck still to be de rusted. Noted work in progress","Deck - Pipe / Fittings","ISM Related","Equipment Related","","","","","Deck pipelined derusting and painting completed","2024-11-30T23:59:35","","Completed","2024-07-20T23:59:35","No","No","No","Internal"]
[null,null,null,37800,54443,"50_Sun Sep 29 2024 03:59:08 GMT+0800","2024-06-15T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Cross lines in cargo manifold area to derust","Deck - Pipe / Fittings","ISM Related","Equipment Related","","","","","cross lines in cargo manifold area  derusted and painted","2024-10-31T23:59:35","","Completed","2024-07-25T23:59:35","No","No","No","Internal"]
[null,null,null,37802,93938,"50_Sun Sep 29 2024 02:44:28 GMT+0800","2024-06-15T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Garbage compactor to clean up and maintain.","Miscellaneous","General Appearance","Equipment Related","","","","","Garbage compactor clean up carried out and maintain on regular basis.","2024-11-30T23:59:35","","Completed","2024-07-20T23:59:35","No","No","No","Internal"]
[null,null,null,37803,19625,"50_Sun Sep 29 2024 02:29:51 GMT+0800","2024-06-15T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Door of wet garbage locker to free up , de-rust and paint.","Miscellaneous","General Appearance","Equipment Related","","","","","Door of wet garbage locker to free up , de-rusting and painting is completed.","2024-11-30T23:59:35","","Completed","2024-07-14T23:59:35","No","No","No","Internal"]
[null,null,null,37804,64887,"50_Sun Sep 29 2024 03:51:48 GMT+0800","2024-06-15T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Steering gear vent on poop deck heavily corroded. to maintain","Deck - Pipe / Fittings","ISM Related","Equipment Related","","","","","Steering gear vent on poop deck derusted and painted","2024-10-31T23:59:35","","Completed","2024-07-20T23:59:35","No","No","No","Internal"]
[null,null,null,37805,79554,"50_Sun Sep 29 2024 04:05:16 GMT+0800","2024-06-15T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Access ladder to foam monitor on deck to descale","Deck - Pipe / Fittings","ISM Related","Equipment Related","","","","","Access ladder to foam monitor on deck descaled and painted","2024-11-30T23:59:35","","Completed","2024-07-27T23:59:35","No","No","No","Internal"]
[null,null,null,37806,53323,"50_Sun Sep 29 2024 04:06:56 GMT+0800","2024-06-15T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Port side bunker manifold midship blanks to derust","Deck - Pipe / Fittings","ISM Related","Equipment Related","","","","","Port side bunker manifold midship blanks  derusted and painted","2024-10-31T23:59:35","","Completed","2024-07-20T23:59:35","No","No","No","Internal"]
[null,null,null,37807,49683,"50_Sun Sep 29 2024 03:02:12 GMT+0800","2024-06-15T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Cargo manifold reducers on stbd side to descale and paint.","Deck - Pipe / Fittings","General Appearance","Equipment Related","","","","","Cargo manifold reducers on stbd side descaling and painting completed.","2024-11-30T23:59:35","","Completed","2024-09-20T23:59:35","No","No","No","Internal"]
[null,null,null,37808,36330,"50_Sun Sep 29 2024 04:09:31 GMT+0800","2024-06-15T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","VRCS Solenoid boxes and save alls on deck require maintainence","Deck - Pipe / Fittings","ISM Related","Equipment Related","","","","","VRCS Solenoid boxes and save alls on deck derusted, painted and maintenance carried out","2024-10-31T23:59:35","","Completed","2024-07-27T23:59:35","No","No","No","Internal"]
[null,null,null,37809,28207,"50_Sun Sep 29 2024 04:03:33 GMT+0800","2024-06-15T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Cargo tank dome cleats and securing arrangements to descale and paint","Deck - Pipe / Fittings","ISM Related","Equipment Related","","","","","Cargo tank dome cleats and securing arrangements  descaled and painted","2024-11-15T23:59:35","","Completed","2024-08-02T23:59:35","No","No","No","Internal"]
[null,null,null,37810,34387,"50_Sun Sep 29 2024 04:11:54 GMT+0800","2024-06-15T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","control air dryer is erratic","E/R - Air Comp.","ISM Related","Equipment Related","","","","","Control air Dryer maintenance carried out and rectified","2024-09-15T23:59:35","","Completed","2024-07-20T23:59:35","No","No","No","Internal"]
[null,null,null,37811,31639,"50_Sun Sep 29 2024 04:20:55 GMT+0800","2024-06-15T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Jacket water controller  is leaking.","E/R - Pipes/ valves & fittings","ISM Related","Equipment Related","","","","","Jacket water controller leak rectified","2024-09-15T23:59:35","","Completed","2024-07-19T23:59:35","No","No","No","Internal"]
[null,null,null,37812,45313,"50_Sun Sep 29 2024 04:28:58 GMT+0800","2024-06-15T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Area around sounding / ullage pipe to be coated with anti Skid Paint. (SIRE Observation on fleet vessel)","Deck - Pipe / Fittings","ISM Related","Equipment Related","","","","","Area around sounding / ullage pipe coated with anti skid paint.","2024-10-31T23:59:35","","Completed","2024-09-29T23:59:35","No","No","No","Internal"]
[null,null,null,37813,78263,"50_Sun Sep 29 2024 04:19:10 GMT+0800","2024-06-15T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Various fresh water line are blanked for fresh water conservation. Fresh water rationing in force  since last one month","Accommodation","ISM Related","Equipment Related","","","","","All fresh water line blanks removed .  Normal supply of fresh water resumed to all areas..","2024-09-15T23:59:35","","Completed","2024-09-21T23:59:35","No","No","No","Internal"]
[null,null,null,37814,75420,"50_Sun Sep 29 2024 04:13:49 GMT+0800","2024-06-15T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Harbor Sea water pump is not in operation","E/R - Pumps","ISM Related","Equipment Related","","","","","Harbor Sea water pump maintenance carried out and made operational","2024-09-15T23:59:35","","Completed","2024-09-10T23:59:35","No","No","No","Internal"]
[null,null,null,37815,71605,"50_Sun Sep 29 2024 04:16:20 GMT+0800","2024-06-15T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Fresh water generator Fresh water inlet & outlet pipe leaking, Repaired with soft patch","E/R - Pipes/ valves & fittings","ISM Related","Equipment Related","","","","","Fresh water generator Fresh water inlet & outlet pipe leak rectified by welding","2024-09-15T23:59:35","","Completed","2024-09-20T23:59:35","No","No","No","Internal"]
[null,null,null,37816,56503,"50_Sun Sep 29 2024 02:55:43 GMT+0800","2024-06-15T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","HFO stbd sounding pipe to de-rust and paint.","Deck - Pipe / Fittings","General Appearance","Equipment Related","","","","","HFO stbd sounding pipe de-rusting and painting completed.","2024-11-30T23:59:35","","Completed","2024-07-27T23:59:35","No","No","No","Internal"]
[null,null,null,36330,57951,"50_Thu Jun 20 2024 03:56:11 GMT+0800","2024-06-15T23:59:35","Breakdown,Observation","Ship Staff","Ship Staff Insp.","Port and Starboard bridge wing rudder angle indicator not operational. Wheelhouse rudder angle indicator has 5 deg error.\n","Navigation - Others","Navigation","Equipment Related","4.7","High","","","Rudder angle indicator troubleshooting and fault rectification carried out as per the technical support.","2024-12-15T23:59:35","","Completed","2024-11-20T23:59:35","No","No","No","Internal","We will arrange service engineer at next call."]
[null,null,null,36331,54554,"50_Thu Jun 20 2024 05:12:21 GMT+0800","2024-06-15T23:59:35","Observation","Ship Staff","Ship Staff Insp.","ME rpm indicator on stbd bridge wing showing inaccurate readings.","Navigation - Others","Navigation","Equipment Related","4.7","High","","","ME RPM INDICATOR STBD SIDE CONNECTIONS MADE AS PER ADVISE FROM MAKER.FOUND WORKING IN ORDER.","2024-11-30T23:59:35","","Completed","2024-10-16T23:59:35","No","No","Yes","Internal"]
[null,null,null,36332,49616,"50_Thu Jun 20 2024 06:51:50 GMT+0800","2024-06-15T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Cargo Eductor gauges in CCR not operational","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","Cargo eductor suction, discharge and drive lines to be  blown through with air. ","2025-03-31T23:59:35","","Completed","2025-01-14T23:59:35","No","No","No","Internal","Noted."]
[null,null,null,36335,65187,"50_Thu Jun 20 2024 05:16:43 GMT+0800","2024-06-15T23:59:35","Non Conformity","Ship Staff","Ship Staff Insp.","Radar image feed not displayed in vdr .","Navigation - VDR / BNWAS","Navigation","Equipment Related","4.7","High","","","Service technician attended at Singapore and rectified the issue.","2025-01-31T23:59:35","","Completed","2024-12-02T23:59:35","No","No","No","Internal","To be attended next call Singapore."]
[null,null,null,36336,15191,"50_Thu Jun 20 2024 06:42:52 GMT+0800","2024-06-15T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Various posters in accommodation area are old versions. To replace with ver 15","Accommodation","Cert. & Docu.","Inappropriate Procedure","","","","","All the posters in accommodation renewed as per the latest revision, sourced from the QDMS.","2024-11-30T23:59:35","","Completed","2024-07-15T23:59:35","No","No","No","Internal","To be connected with joiners."]
[null,null,null,36337,21035,"50_Thu Jun 20 2024 06:44:29 GMT+0800","2024-06-15T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Steering gear vent on poop deck heavily corroded. ","Miscellaneous","General Appearance","External Factors","","","","","Steering gear vent on poop deck, de-rusting and painting completed.","2024-08-15T23:59:35","","Completed","2024-06-27T23:59:35","No","No","No","Internal"]
[null,null,null,36339,66743,"50_Thu Jun 20 2024 06:46:34 GMT+0800","2024-06-15T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Numerous sections of ship side railings on deck corroded. ","Miscellaneous","General Appearance","External Factors","","","","","Ship side railings de rusting and painting is completed.","2024-08-31T23:59:35","","Completed","2024-07-30T23:59:35","No","No","No","Internal"]
[null,null,null,36341,54216,"50_Thu Jun 20 2024 06:49:29 GMT+0800","2024-06-15T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","IG line flanges on main deck in poor condition","","General Appearance","External Factors","","","","","De-rusting and painting of IG line flanges is completed.","2024-09-15T23:59:35","","Completed","2024-08-10T23:59:35","No","No","No","Internal"]
[null,null,null,36342,23121,"50_Thu Jun 20 2024 06:48:18 GMT+0800","2024-06-15T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Foam monitors on deck to be upgraded. Safety items ","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","De-rusting and painting of foam monitors is completed.","2024-09-15T23:59:35","","Completed","2024-08-10T23:59:35","No","No","No","Internal"]
[null,null,null,36343,23340,"50_Thu Jun 20 2024 06:41:28 GMT+0800","2024-06-15T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","No 2 Life Boat hatch rubber packing is damaged and loose. Rain water ingress into boat ","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","Rubber Packing renewed and checked the condition inside the lifeboat. All found in good order.","2024-06-30T23:59:35","","Completed","2024-06-17T23:59:35","No","No","No","Internal"]
[null,null,null,37801,28047,"50_Sun Sep 29 2024 04:01:46 GMT+0800","2024-06-16T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Step ladder to Starboard manifold drip tray to replace corroded and sharp edge step","Deck - Pipe / Fittings","ISM Related","Equipment Related","","","","","Step ladder to Starboard manifold drip tray  replaced the corroded and sharp edge step","2024-10-31T23:59:35","","Completed","2024-09-07T23:59:35","No","No","No","Internal"]
[null,null,null,33812,18279,"50_Sat Feb 03 2024 06:41:26 GMT+0800","2024-06-20T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Both AHU Units supply air and return air operating levers for flaps found in broken condition.","Accommodation","Eng. / Strg. Comp.","Equipment Related","","","","","New operating levers fabricated for AHU 1 fresh air intake.All other supply and return operating levers eased up.","2024-09-30T23:59:35","","Completed","2024-09-18T23:59:35","No","No","No","Internal","Spares are on order."]
[null,null,null,36745,60622,"50_Tue Jul 16 2024 21:00:33 GMT+0800","2024-07-13T23:59:35","Defect","Ship Staff","Ship Staff Insp.","3P WBT vent head corroded and damaged.","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","Equipment Related","","","","","During maintenance, it was found that 3P WBT vent head is corroded and damaged. Removed and fabrication completed. ","2024-08-15T23:59:35","","Completed","2024-07-26T23:59:35","No","No","No","Internal"]
[null,null,null,36733,61682,"50_Tue Aug 06 2024 07:36:58 GMT+0800","2024-07-15T23:59:35","Defect","Ship Staff","Ship Staff Insp.","PORT LIFEBOAT MOTOR WAS BURNT DUE TO AGEING EFFECT , IT IS BEYONG REPAIR ","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","RECIEVED THE REQUISITION RAISED : DPEO240170-MOTOR COMPLETE FOR PORT SIDE LIFEBOAT/RESCUE BOAT DAVIT WINCH , TESTED , NOW OK ","2024-08-15T23:59:35","DPEO240170-MOTOR COMPLETE FOR PORT SIDE LIFEBOAT/RESCUE BOAT DAVIT WINCH","Completed","2024-08-08T23:59:35","No","No","No","Internal"]
[null,null,null,36737,39116,"50_Tue Aug 06 2024 08:45:40 GMT+0800","2024-07-15T23:59:35","Defect","Ship Staff","Ship Staff Insp.","SOME OF THE BUNKER MANIFLD PRESSURE GAUGE CABINET DOORS ARE IN DAMAGED CONDITION AT THE MANIFOLD AREA , CAUSING UNABLE TO CLOSE THEM WHICH CAN LEAD TO CORROSION / LEAK FROM PRESSURE GAUGE CONNECTIONS IN LONG RUN","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","External Factors,Equipment Related","","","","","Cabinets repaired and now positively closing.","2024-09-30T23:59:35","","Completed","2024-09-24T23:59:35","No","No","Yes","Internal","Update the present status."]
[null,null,null,36741,54901,"50_Tue Aug 06 2024 08:51:50 GMT+0800","2024-07-15T23:59:35","Defect,Other","Ship Staff","Ship Staff Insp.","IT WAS OBSERVED THAT AFT MOORING COOLER WAS LEAKING FOR VERY LONG TIME , THIS HAS CAUSED WATER/ SALT CONTAMINATION OF AFT MOORING OIL IN THE PAST ","","Eng. / Strg. Comp.","Human Error,Equipment Related","","","","","NEW COOLER RECIEVED & FITTED , TESTED THE SAME , TANK & SYSTEM DRAINED / now oil quality is ok ","2024-08-20T23:59:35","","Completed","2024-08-11T23:59:35","No","No","No","Internal"]
[null,null,null,36744,44249,"50_Tue Jul 16 2024 20:57:31 GMT+0800","2024-07-15T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Leak at motor connection on port side gangway.","Deck - Machinery","Mooring","Equipment Related","","","","","It was observed that there was a leak from motor connection on port side gangway. To be rectified. The circlip at the motor connection renewed. We will verify the rectification during operation.","2024-08-15T23:59:35","","Completed",null,"No","No","No","Internal"]
[null,null,null,36734,21330,"50_Tue Aug 06 2024 11:14:30 GMT+0800","2024-07-16T23:59:35","Observation,Non Conformity","Ship Staff","Ship Staff Insp.","EMERGENCY STORE DESIGNATED BOX NOT MADE & EMERGENCY STORES NOT AVAILABLE , AS PER GOODWOOD POLICY","Miscellaneous","Emgcy. Systems","Inappropriate Procedure","","","","","RAISED REQUISITION FOR EMERGENCY STORES AS PER GOODWOOD POLICY AND RECIEVED ON 01-12-2024.SHIP STAFF FABRICATED A BOX FOR EMERGENCY STORES AND KEPT ITEMS IN THAT AFTER COLOUR CODING.","2024-12-31T23:59:35","DPEO240202","Completed","2024-12-23T23:59:35","No","No","Yes","Internal"]
[null,null,null,36730,12617,"50_Tue Aug 06 2024 07:29:31 GMT+0800","2024-08-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","STARBOARD SIDE GANGWAY PORT FORWARD WHEEL BEARING & WHEEL IS IN DAMAGED CONDITION","Deck - Machinery","Structural Condn. / WT integrity ","Equipment Related","","","","","STBD GANGWAY ROLLERS 2 NOS BEARINGS RENEWED.THE REMAINING 2 NOS WILL BE RENEWED AT SEA\nBoth gangway wheels bearings renewed. Gangway tested satisfactorily","2024-12-31T23:59:35","DPEO240239","Completed","2024-12-18T23:59:35","No","No","No","Internal","As discussed at suitable opportunity we will attend it as it require hotwork."]
[null,null,null,36731,41943,"50_Tue Aug 06 2024 07:32:08 GMT+0800","2024-08-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","PORT MISDHIP CRANE LIMIT SWITCH NEED TO BE RENEWED AS GIVING ISSUES SOMETIMES","Deck - Machinery","Safety / LSA / FFA","Equipment Related","","","","","LIMIT SWITCH FOR THE PORT SIDE HHC HAS BEEN RENEWED ON 25 SEP 2024, AT SEA. AFTER TESTING THE OPERATION IS WAS OBSERVED THAT THERES IS STILL A DELAY IN RUNNER WIRE OPEARTION,TECHNICIAN ATTENDED THE VESSEL AND FOUND THAT THE COUNTERBALANCE VALVE SETTING WAS FAULTY.SAME ADJUSTED.","2024-12-15T23:59:35","","Completed","2024-12-01T23:59:35","No","No","No","Internal","Plan for this job at this anchorage."]
[null,null,null,36732,35621,"50_Tue Aug 06 2024 07:34:45 GMT+0800","2024-08-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","STARBOARD LIFEBOAT NOTICED THAT THE CHARGER IS ERRATIC AS IT IS ABLE TO CHARGE ONLY 1 BATTERY , BATTERIES ARE OK , THERE IS NO CHARGING LIGHT COMING ON THE SECOND BATTERY SHOWING RED INDICATION","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","Battery charger recieved and fitted to stbd lifeboat.Found charging in order.","2024-12-15T23:59:35","REQUISITION RAISED : DPEO240189-LIFEBOAT BATTERY CHARGER","Completed","2024-11-15T23:59:35","No","No","Yes","Internal","Till the charger is not supplied, keep on charging the battery externally on regular basis."]
[null,null,null,36735,67341,"50_Tue Aug 06 2024 08:48:22 GMT+0800","2024-08-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","NOTICED THE BATTERY CHARGER FOR SAAB TANK GAUGING SYSTEM IN CCR IS ERRATIC","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","TEMPORARILY PORTABLE CHARGER HAS BEEN PLACED THERE , REQUISITION RAISED : DPEO240186-BATTERY CHARGER FOR REMOTE TANK GAUGING SYSTEM AND SAME RENEWED ON 01-12-2024","2024-12-15T23:59:35","DPEO240186-BATTERY CHARGER FOR REMOTE TANK GAUGING SYSTEM","Completed","2024-12-01T23:59:35","No","No","No","Internal","Noted."]
[null,null,null,36738,81938,"50_Tue Aug 06 2024 08:40:49 GMT+0800","2024-08-01T23:59:35","Other","Ship Staff","Ship Staff Insp.","HOUSEKEEPING OF VARIOUS VENT HEADS AND ALSO INCLUDING THOSE OF BUNKER TANKS /BUNKER LINE & VALVES NEED PAINTING & HOUSEKEEPING","Deck - Machinery","General Appearance","External Factors","","","","","VENT HEADS OVERHAULED ,  REPAIRED THE DAMAGED PLATED / PAINTING & HOUSEKEEPING OF SAME CARRIED OUT","2024-09-30T23:59:35","","Completed","2024-09-12T23:59:35","No","No","Yes","Internal","Update in weekly report."]
[null,null,null,36739,76397,"50_Tue Aug 06 2024 08:38:48 GMT+0800","2024-08-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","PERFORMANCE OF ATMOSPHERIC CONDENSERS IS NOT GOOD CAUSING STEAMING EVEN THOUGH BYPASS IS SHUT ","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Both atmospheric condensers cleaned one by one , anodes renewed also , end sections were corroded , same repaired by bringing to workshop & built up ","2024-08-15T23:59:35","","Completed","2024-08-12T23:59:35","No","No","No","Internal"]
[null,null,null,36740,29846,"50_Tue Aug 06 2024 07:39:54 GMT+0800","2024-08-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","SERVICE AIR COMPRESSOR NOT IN USE FOR SOMETIME DUE TO AWAITED OIL SEAL , THIS IS CAUSING MORE RUNNING HRS OF MAIN COMPRESSORS ESPECIALLY DURING DECK MAINTENANCE","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related","","","","","oil seal recieved on 01-12-2024.Fitted on compressor and tried out.Found running in order without any leaks.","2024-12-31T23:59:35","DPEO240093-SERVICE AIR COMPRESSOR SEAL","Completed","2024-12-20T23:59:35","No","No","No","Internal","Spares ready, will be connected next call."]
[null,null,null,36742,48790,"50_Tue Aug 06 2024 07:44:15 GMT+0800","2024-08-01T23:59:35","Defect,Observation,Other","Ship Staff","Ship Staff Insp.","IT HAS BEEN OBSERVED THAT MANY OF THE DRAINS FROM DG 3 SAVEALLS & NEARBY OIL TRAYS IS CONNECTED TO CLEAN DRAIN TANK WHICH SHIP STAFF WAS NOT AWARE , THESE TO BE EITHER BLANKED OR RE ROUTED THROUGH TO WASTE OIL TANK TO PREVENT CONTAMINATION OF CLEAN DRAIN TANK ( AS ORIGINALLY AT THE PLACE OF DG 3 THERE WAS TURBO GENERATOR & STEAM PLANT )","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Inappropriate Procedure","","","","","FOR THE TIME BEING WE HAVE BLANKED THE OILY LINE GOING TO CLEAN DRAIN TANK BUT THIS IS A TEMPORARY SOLUTION","2024-09-30T23:59:35","","Completed","2024-08-27T23:59:35","No","No","No","Internal","Plan for the modification and share the plan"]
[null,null,null,36743,17903,"50_Tue Aug 06 2024 07:48:27 GMT+0800","2024-08-01T23:59:35","Other","Ship Staff","Ship Staff Insp.","DUE TO SHIP'S LONG ANCHORAGE IN LAST 3 MONTHS , VESSEL HAS BEEN ON LONG FW RATIONING AS THERE IS NO OTHER OPTION , WE HAVE RECTIFIED MANY MANY LEAKS IN PAST & FWG PRODUCTION IS ALSO NOW INCREASED BUT THIS IS THE ONLY OPTION TO KEEP RATIONING , WE COLLECTING AC CONDENSATE ALSO","Miscellaneous","MLC Related","External Factors","","","","","FWG Running to make up for water shortage","2024-10-01T23:59:35","","Completed","2024-08-31T23:59:35","No","No","Yes","Internal"]
[null,null,null,36746,59429,"50_Tue Aug 06 2024 07:41:30 GMT+0800","2024-08-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","STEERING GEAR ROOM EXHAUST FAN DAMPER WAS FROZEN & WAS IN VERY POOR CONDITION ","Deck - Machinery","Structural Condn. / WT integrity ","Equipment Related","","","","","SAME HAS BEEN REPAIRED & PAINTED , NOW OK , ONLY THE LADDER NEED REPAIRS ","2024-08-10T23:59:35","","Completed","2024-08-01T23:59:35","No","No","No","Internal"]
[null,null,null,37152,42078,"50_Tue Sep 03 2024 07:41:56 GMT+0800","2024-08-15T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Soot tank outlet line to overboard has soft patch.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Pipe renewed after seeking concurrence for hot work from office","2024-10-15T23:59:35","","Completed","2024-10-02T23:59:35","No","No","No","Internal"]
[null,null,null,37140,72504,"50_Tue Sep 03 2024 07:05:43 GMT+0800","2024-08-16T23:59:35","Defect","Ship Staff","Ship Staff Insp.","ME crank angle sensor no:1 is not showing any output in the RPLS Panel in ECR,\n","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","ME crank angle sensor no:1 and controlle box renewed.The sensor wheel slots cleaning carried out. and sensor adjusted.Sensor tested by rotating the engine and found crank angle changing.","2024-12-15T23:59:35","","Completed","2024-12-01T23:59:35","No","No","No","Internal"]
[null,null,null,37143,84000,"50_Tue Sep 03 2024 07:24:51 GMT+0800","2024-08-17T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Emergency fire pump suction and discharge valves found passing","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Ship staff has recieved the suction and discharge valves.Discharge valve renewed and suction valve found holding.","2024-09-18T23:59:35","","Completed","2024-09-06T23:59:35","No","No","No","Internal"]
[null,null,null,37420,54329,"50_Tue Sep 17 2024 07:11:01 GMT+0800","2024-08-17T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Emergency fire pump suction and discharge valves found passing","E/R - Pumps","","Equipment Related","","","","","Emergency fire pump discharge valve renewed and suction valve checked and found passing.","2024-09-30T23:59:35","","Completed","2024-09-04T23:59:35","No","No","No","Internal"]
[null,null,null,37144,28294,"50_Tue Sep 03 2024 07:19:10 GMT+0800","2024-08-19T23:59:35","Defect","Ship Staff","Ship Staff Insp.","AC compressor no:1 capacity control is faulty and hence the compressor units are not coming on load.\n","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Capacity control hydraulic relay found sticking.Same overhauled.The mechinical linkages checked and found sticking.Same overhauled ,boxed back and AC compressor tried out.Found working in order.\n","2024-09-19T23:59:35","","Completed","2024-09-02T23:59:35","No","No","No","Internal"]
[null,null,null,37154,57226,"50_Tue Sep 03 2024 07:10:11 GMT+0800","2024-08-19T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Incinerator exhaust gas fan is observed having a high level of vibration\n","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Incinerator blower opened and checked that the shaft trueness and blower trueness are on the higher side.Shaft and blower renewed with spare new.axial wobble checked and found in order.Incinerator tried and found working satisfactory.\n","2024-09-02T23:59:35","","Completed","2024-08-29T23:59:35","No","No","No","Internal"]
[null,null,null,37139,93838,"50_Tue Sep 03 2024 07:22:31 GMT+0800","2024-08-20T23:59:35","Defect","Ship Staff","Ship Staff Insp.","AE3 Unit no:1 and 3 temperture sensor faulty.\n","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","AE3 unit 1 and 3 temperature sensor checked by temperature calibrator and found faulty.RO DPEO240018 placed for the same and recieved on 01-12-2024.Ship staff has carried out renewal of sensor and cable.Found working in order.\n","2024-12-31T23:59:35","DPEO240018","Completed","2024-12-10T23:59:35","No","No","No","Internal"]
[null,null,null,37142,17080,"50_Tue Sep 03 2024 07:35:04 GMT+0800","2024-08-20T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Vacuum condenser level controller not working in AUTO","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Vacuum condenser level controller orifice was found  chocked.Same was renewed.The positioner overhaul carried out.Level controlled tried out and is now maintain the level in auto.","2024-12-15T23:59:35","","Completed","2024-12-01T23:59:35","No","No","No","Internal"]
[null,null,null,37146,99658,"50_Tue Sep 03 2024 07:49:26 GMT+0800","2024-08-20T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Fresh water generator performance is poor.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Manaul cleaning of fresh water generator tubes carried out.Demister and condenser cleaning carried out.After cleaning the fresh water production is 25MT.","2024-09-30T23:59:35","","Completed","2024-09-23T23:59:35","No","No","No","Internal"]
[null,null,null,37149,54482,"50_Tue Sep 03 2024 07:55:56 GMT+0800","2024-08-20T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Main air compressor No:3 LO pressure switch faulty","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","RO placed for a new pressure switch is recieved on 1-12-2024.Same fitted to compressor an tried out.Found in good order.","2024-12-15T23:59:35","DPEO240194","Completed","2024-12-15T23:59:35","No","No","No","Internal"]
[null,null,null,37137,24337,"50_Tue Sep 03 2024 07:21:13 GMT+0800","2024-08-21T23:59:35","Defect","Ship Staff","Ship Staff Insp.","HFO Bunker tank No:2 HFO tk,HFO 1S Tank,HFO No:1 service tank and various other Dip trays found wasted. \n","Deck - Pipe / Fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Bunker tanks drip trays cold work repair completed.All drip trays painted after repair","2024-09-30T23:59:35","","Completed","2024-09-24T23:59:35","No","No","No","Internal"]
[null,null,null,37141,59443,"50_Tue Sep 03 2024 07:28:42 GMT+0800","2024-08-22T23:59:35","Observation","Ship Staff","Ship Staff Insp.","During IG top up it was observed that the vacuum condenser bottom surface is getting very hot.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Vacuum condenser tubes cleaning carried out.Found many tubes chocked with shells.All the tubes cleared and fitted with new anodes.","2024-09-30T23:59:35","","Completed","2024-09-27T23:59:35","No","No","No","Internal"]
[null,null,null,37148,43827,"50_Tue Sep 03 2024 08:09:40 GMT+0800","2024-08-22T23:59:35","Defect","Ship Staff","Ship Staff Insp.","440V low insulation alarm is triggered when running icolube.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Isolation transformer fitted to icolube system.440V low isulation alarm is not triggered now.","2024-11-30T23:59:35","","Completed","2024-11-20T23:59:35","No","No","No","Internal"]
[null,null,null,37153,45787,"50_Tue Sep 03 2024 08:12:35 GMT+0800","2024-08-22T23:59:35","Defect","Ship Staff","Ship Staff Insp.","LO purifier no:1  EPC is not working ","E/R - Purifier","","Equipment Related","","","","","vessel recieved the new EPC on 01-12-2024.Same will be fitted and installation carried out.Found working in order","2025-01-31T23:59:35","RO DPEO240136","Completed","2024-12-17T23:59:35","No","No","No","Internal"]
[null,null,null,37150,12714,"50_Tue Sep 03 2024 08:17:39 GMT+0800","2024-08-23T23:59:35","Defect","Ship Staff","Ship Staff Insp.","IS TGU suspected faulty as there is no parameters indication for the 1S tank in the panel","Hull & Tanks","Eng. / Strg. Comp.","Equipment Related","","","","","CHECKS CARRIED OUT AND FOUND THAT THE TGU IS FAULTY.VESSEL HAS PLACED RO DPEO240269 FOR THE SAME.\nTGU REPLACED BY SERVICE TECHNICIAN AT SINGAPORE. SYSTEM TESTED , 1 STBD TGU WORKING SATISFACTORILY","2024-12-15T23:59:35","DPEO240269","Completed","2024-12-03T23:59:35","No","No","No","Internal"]
[null,null,null,37151,60994,"50_Tue Sep 03 2024 08:20:17 GMT+0800","2024-08-29T23:59:35","Defect","Ship Staff","Ship Staff Insp.","BNWAS port bridge wing reset button damaged","Navigation - VDR / BNWAS","Eng. / Strg. Comp.","Equipment Related","","","","","RO DPEO240235 placed for a new push button  was recieved in singapore on 01-12-2024.Ship staff is in process of renewing the push button.\nSwitch replaced with spare received. System tested working satisfactorily","2024-12-31T23:59:35","DPEO240235","Completed","2024-12-18T23:59:35","No","No","No","Internal",""]
[null,null,null,37138,13519,"50_Tue Sep 03 2024 07:12:17 GMT+0800","2024-08-30T23:59:35","Defect","Ship Staff","Ship Staff Insp.","No:1 and 2 Boiler feed water valves main and auxiliary found passing","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","Boiler feed water valve 4 nos main and aux. positioner calibrated and valve found operating in order.","2024-11-30T23:59:35","","Completed","2024-12-01T23:59:35","No","No","No","Internal"]
[null,null,null,37419,62057,"50_Tue Sep 17 2024 07:05:23 GMT+0800","2024-09-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","GPS communication fault alarm showing in the EGCS Panel.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","EGCS GPS feed is now showing in EGCS panel.The PLC settings for the repeater changed.","2024-10-30T23:59:35","","Completed","2024-10-21T23:59:35","No","No","No","Internal"]
[null,null,null,37416,12866,"50_Tue Sep 17 2024 07:03:17 GMT+0800","2024-09-09T23:59:35","Defect","Ship Staff","Ship Staff Insp.","IG Scrubber overboard line found holed and wasted/thinned down","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Overboard line pipe fabrication completed.Pipe fitted in place and scrubber pump started.Found no leaks","2024-09-30T23:59:35","","Completed","2024-09-13T23:59:35","No","No","No","Internal"]
[null,null,null,37417,56100,"50_Tue Sep 17 2024 07:01:46 GMT+0800","2024-09-11T23:59:35","Defect","Ship Staff","Ship Staff Insp.","The steam line on main deck provided for Mast Riser firefighting is heavily corroded and few sections are wasted.","Deck - Pipe / Fittings","General Appearance","Equipment Related","","","","","Wasted sections renewed.","2025-03-31T23:59:35","DPEO240227","Completed","2025-01-30T23:59:35","No","No","No","Internal"]
[null,null,null,37780,78511,"50_Wed Oct 16 2024 02:56:03 GMT+0800","2024-09-20T23:59:35","Defect","Ship Staff","Ship Staff Insp.","ONE HERMATIC UTI / MMC NOT OPERATIONAL.","Critical Equip.","Cargo / Ballast Systems","Equipment Related","8.30","High","","","REQUISITION RAISED FOR THE REAPAIRS AND SERVICE. REQ NO. DPEO240263","2024-11-30T23:59:35","DPEO240263","Completed","2024-10-17T23:59:35","No","No","No","Internal"]
[null,null,null,38322,46387,"50_Mon Oct 28 2024 10:20:21 GMT+0800","2024-09-25T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Elevator non operational","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","Elevator control panel,travelling cable,local control panel renewed.The limit switched of each decks checked.Elevator tried out and found in order.","2024-12-31T23:59:35","","Completed","2024-12-01T23:59:35","No","No","No","Internal"]
[null,null,null,37778,23014,"50_Mon Oct 14 2024 12:40:43 GMT+0800","2024-10-11T23:59:35","Observation","Ship Staff","Ship Staff Insp.","CALIBRATION CERTIFICATE FOR MOORING WINCH BRAKE TESTING KIT HYDRAULIC JACK PRESSURE GAUGE, NOT AVAILABLE ONBOARD.","Deck - Mooring Machinery","Mooring","Equipment Related","","","","","SERVICE REQUISTION RAISED FOR THE BRC TEST KIT HYDRAULIC JACK PRESSURE GAUGE CALIBRATION.   REQ NO. DPEO240264\nCalibration carried out at on 30 Nov 2024","2024-12-31T23:59:35","DPEO240264","Completed","2024-11-30T23:59:35","No","No","No","Internal"]
[null,null,null,38317,35926,"50_Sun Dec 15 2024 13:35:20 GMT+0800","2024-10-14T23:59:35","Defect","Ship Staff","Ship Staff Insp.","HFO Purifier no:2 I/O Card not working.","E/R - Purifier","Eng. / Strg. Comp.","Equipment Related","","","","","HFO Purifier no:2 I/O Card  working.","2025-01-31T23:59:35","DPEO240323","Completed","2024-12-17T23:59:35","No","No","No","Internal"]
[null,null,null,37779,46851,"50_Tue Oct 15 2024 08:29:05 GMT+0800","2024-10-15T23:59:35","Observation","Ship Staff","Ship Staff Insp.","CARGO MANIFOLD BOLTS ARE SHORT IN LENGTH.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.41","Medium","","","CARGO MANIFOLD BOLTS ARE SHORT IN LENGTH, AS COMPARED TO VIQ REQUIREMENT OF HAVING 3-4 THREAD VISIBLE AFTER TIGHTINING THE BOLTS. REQUISITION RAISED FOR THE REQUIRED BOLT AND NUTS. REQ NO- DPEO240272\nManifold bolts replaced with spares. Now in correct length","2024-12-31T23:59:35","DPEO240272","Completed","2024-12-14T23:59:35","No","No","No","Internal"]
[null,null,null,37781,50447,"50_Fri Oct 18 2024 09:29:34 GMT+0800","2024-10-16T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","Stbd Side hose handling crane limit switch not working","Deck - Machinery","Cargo / Ballast Systems","Equipment Related","","","","","RO raised DPEO240274 and recieved.Limit switch renewed.","2025-01-15T23:59:35","","Completed","2024-12-26T23:59:35","No","No","No","Internal"]
[null,null,null,38316,27243,"50_Sun Dec 15 2024 13:39:36 GMT+0800","2024-10-16T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Engine room crane electronic limit is not operational","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","RO DPEO 240232 placed for a spare limit switch and recieved in singapore on 01-12-2024.same renewed and tried out.working in order","2024-12-31T23:59:35","DPEO240232","Completed","2024-12-26T23:59:35","No","No","No","Internal"]
[null,null,null,37782,95388,"50_Sat Oct 19 2024 10:15:34 GMT+0800","2024-10-18T23:59:35","Defect","Ship Staff","Ship Staff Insp.","VISUAL ALARM / STRAUB LIGHT FOR PUMP ROOM GAS DETECTION SYSTEM NOT WORKING IN PUMP ROOM.","Cargo Mach.","Emgcy. Systems","Equipment Related","","","","","IT WAS OBSERVED THAT THE STRAUB LIGHT FOR PUMP ROOM FIXED GAS DETECTION SYSTEM IN PUMP ROOM, IS NOT WORKING/ FUSED. RO WILL BE RAISED FOR NEW STRAUB LIGHT.\nPump room HC alarm light replaced from spares Received. Audio visual alarm tested working satisfactory","2024-11-30T23:59:35","","Completed","2024-12-27T23:59:35","No","No","No","Internal"]
[null,null,null,38321,61123,"50_Sun Dec 15 2024 13:42:57 GMT+0800","2024-10-29T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","Boiler no:1 feed pump found not developing pressure.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","","","","","Pump dismantled and found that the impellers 1st and 3rd stage were broken.Ship staff carried out the overhaul of the pump and tried out.Working in order.","2024-12-15T23:59:35","","Completed","2024-12-14T23:59:35","No","No","No","Internal"]
[null,null,null,38319,20746,"50_Sun Dec 15 2024 13:45:52 GMT+0800","2024-12-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Fuel oil inlet to main engine temperature sensor showing error.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","The temperature sensor and the cabling checks will be carried out.\nVessel has layed down the separate 3 core armoured cable for the sensor and working satisfactory.","2025-01-31T23:59:35","","Completed","2025-01-03T23:59:35","No","No","No","Internal"]
[null,null,null,38323,30358,"50_Sun Dec 15 2024 13:47:57 GMT+0800","2024-12-01T23:59:35","Observation","Ship Staff","Suptd. Insp.","Lo purifier no:2 temperature not maintaining 90-95 deg upon observation by superitendent.","E/R - Purifier","Eng. / Strg. Comp.","Equipment Related","","","","","Ship staff carried out the adjustment of the temperature setting and also placed a notice that 90-95 deg to be maintained at the inlet to purifier.","2024-12-15T23:59:35","","Completed","2024-12-10T23:59:35","No","No","No","Internal"]
[null,null,null,38888,81322,"50_Sat Dec 21 2024 12:10:21 GMT+0800","2024-12-01T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","OIL POT MISSING FROM NO:2 HP CIRCULATING PUMP.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","","","","","OIL POT TO BE FITTED IN PLACE TO THE NO:2 HP CIRULATING PUMP","2024-12-31T23:59:35","","Completed","2024-12-18T23:59:35","No","No","No","Internal"]
[null,null,null,38890,14423,"50_Sat Dec 21 2024 12:06:21 GMT+0800","2024-12-01T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","LT COOLER SPARE NEW GASKETS TO BE SHIFTED TO AC ROOM TO AVOID GETTING BRITTLE","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","LT COOLER GASKETS KEPT IN ENGINE ROOM SPARE PART SPACE TO BE SHIFTED TO AC ROOM TO AVOID  GETTING BRITTLE","2024-12-31T23:59:35","","Completed","2024-12-17T23:59:35","No","No","No","Internal"]
[null,null,null,38891,22702,"50_Sat Dec 21 2024 12:12:23 GMT+0800","2024-12-01T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","LAGGING MISSING FROM THE BOTH MANHOLE COVER OF BOILER NO:1 AND 2","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","LAGGING PLACED TO THE MANHOLE COVER DOORS OF BOILER NO:1 AND 2","2024-12-31T23:59:35","","Completed","2024-12-20T23:59:35","No","No","No","Internal"]
[null,null,null,38908,46802,"50_Sun Dec 22 2024 14:37:12 GMT+0800","2024-12-01T23:59:35","Observation","Ship Staff","Ship Staff Insp.","All AE'S kwh meter to be renewed with new supplied ones","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","As in the present ones,the power to the meter gets switched off when the AE is stopped,the newly supplied kwh meters to be installed after seeking concurrence from autoelec department.","2025-01-31T23:59:35","","Completed","2025-01-03T23:59:35","No","No","No","Internal"]
[null,null,null,38910,23550,"50_Sat Dec 21 2024 12:04:13 GMT+0800","2024-12-01T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ENGINE ROOM BLOWERS FLAPS MAINTENANCE TO BE CARRIED OUT AS FOUND RUSTED.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","ENGINE ROOM BLOWER FLAPS TO BE DISMANTLED AND DAMAGED PLACES TO BE REPAIRED BY HOT HOT WORK IN WORKSHOP.AFTER REPAIR IT IS TO BE PAINTED BY PRIMER AND FITTED BACK.NO:2 VENT FAN FLAPS ARE COMPLETED.WORK IN PROGRESS ","2025-01-15T23:59:35","","Completed","2025-01-02T23:59:35","No","No","No","Internal"]
[null,null,null,38876,99896,"50_Wed Dec 18 2024 13:07:43 GMT+0800","2024-12-02T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","The door packing of both lifeboat to be renewed as highlighted during annual Survey.","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.28","Very High","","","Door packing of both Lifeboats replaced with new packing","2024-12-22T23:59:35","","Completed","2024-12-06T23:59:35","No","No","No","Internal"]
[null,null,null,38877,85509,"50_Wed Dec 18 2024 13:10:26 GMT+0800","2024-12-02T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","High press hose of both windlass hydraulic brake cylinder to renew as fitting are in bad condition.","Deck - Mooring Machinery","Mooring","Equipment Related","9.20","Medium","","","high press hoses renewed with spares onboard","2024-12-17T23:59:35","","Completed","2024-12-17T23:59:35","No","No","No","Internal"]
[null,null,null,38878,49682,"0_Sun Dec 29 2024 10:41:39 GMT+0800","2024-12-02T23:59:35","Non Conformity","Owner / Marine / Tech. Suptd.","ISM Audit","ALL LIFE JACKETS ONBOARD WERE OLDER THAN 10 YEARS","LSA / FFA","Safety / LSA / FFA","Human Error","","","","","new lifejacket received and put in use","2025-03-01T23:59:35","","Completed","2024-12-05T23:59:35","No","No","No","Internal"]
[null,null,null,38879,16693,"0_Sun Dec 29 2024 10:46:05 GMT+0800","2024-12-02T23:59:35","Non Conformity","Owner / Marine / Tech. Suptd.","ISM Audit","APPENDIX 1 - CONTACT INFORMATION (FLAG SPECIFIC) - 08.90.00.00 - IS OF OLDER VERSION (18.5.2021). NEWER VERSION IS DATED 01.03.2024 (08.90.02.00.A01)","Documentation","Cert. & Docu.","Human Error","","","","","OLDER VERSION (18.5.2021) UPDATED WITH NEWER VERSION DATED 01.03.2024 (08.90.02.00.A01)","2025-03-01T23:59:35","","Completed","2024-12-05T23:59:35","No","No","No","Internal"]
[null,null,null,38880,82141,"50_Sun Dec 29 2024 10:49:46 GMT+0800","2024-12-02T23:59:35","Observation","Owner / Marine / Tech. Suptd.","ISM Audit","CERTIFICATES FOLDER HAS OLDER/EXPIRED CERTIFICATES/ SERVICE REPORTS. TO UPDATE WITH ONLY RELEVANT CERTIFICATES/ SERVICE REPORTS","Documentation","Cert. & Docu.","Human Error","","","","","CERTIFICATES FOLDER / SERVICE REPORTS UPDATED WITH THE RELEVANT  CERTIFICATES/ SERVICE REPORTS","2025-03-01T23:59:35","","Completed","2024-12-06T23:59:35","No","No","No","Internal"]
[null,null,null,38881,33921,"50_Sun Dec 29 2024 10:38:44 GMT+0800","2024-12-02T23:59:35","Non Conformity","Owner / Marine / Tech. Suptd.","ISM Audit","ONLY ONE VENDOR FAMILIARIZATION NOTED ONBOARD; THERE WERE MUTLIPLE SHORE SERVICE ATTENDACE ON 01/12 AND 02/12.","Documentation","Cert. & Docu.","Behaviour Based","","","","","Form completed","2025-03-01T23:59:35","","Completed","2024-12-04T23:59:35","No","No","No","Internal"]
[null,null,null,38882,59354,"0_Sun Dec 29 2024 10:52:42 GMT+0800","2024-12-02T23:59:35","Non Conformity,Observation","Owner / Marine / Tech. Suptd.","ISM Audit","BIO FOULING RECORD BOOK, SEC 4 HAS SCREEN SHOTS FROM PAL 3.0. SAME TO BE UPDATED WITH PAL 4.0 PROCEDURES.","Documentation","Cert. & Docu.","Human Error","","","","","BIO FOULING RECORD BOOK, SEC 4 UPDATED WITH PAL 4.0 PROCEDURES","2025-03-01T23:59:35","","Completed","2024-12-06T23:59:35","No","No","No","Internal"]
[null,null,null,38883,59024,"0_Sun Dec 29 2024 11:17:10 GMT+0800","2024-12-02T23:59:35","Observation","Owner / Marine / Tech. Suptd.","ISM Audit","EYE WASH IN ER WORKSHOP COVERED WITH DUST","Miscellaneous","General Appearance","External Factors","","","","","EYE WASH IN ER WORKSHOP CLEANED","2025-03-01T23:59:35","","Completed","2024-12-05T23:59:35","No","No","No","Internal"]
[null,null,null,38884,72623,"0_Sun Dec 29 2024 11:27:16 GMT+0800","2024-12-02T23:59:35","Observation","Owner / Marine / Tech. Suptd.","MLC Audit","ER TOILET IS VERY UNTIDY AND UNUSABLE","Accommodation","Eng. / Strg. Comp.","Behaviour Based","","","","","ER TOILET CLEANED ON DAILY BASIS","2025-03-01T23:59:35","","Completed","2024-12-05T23:59:35","No","No","No","Internal"]
[null,null,null,38885,19948,"50_Sun Dec 29 2024 11:00:48 GMT+0800","2024-12-02T23:59:35","Observation","Owner / Marine / Tech. Suptd.","ISM Audit","TO MARK PORT AND STARBOARD AT THE EMERGENCY STEERING OPERATOR STAND","Miscellaneous","Emgcy. Systems","Knowledge Based","","","","","PORT AND STARBOARD SIDE  MARKED AT THE EMERGENCY STEERING OPERATOR STAND","2025-01-31T23:59:35","","Completed","2024-12-28T23:59:35","No","No","No","Internal"]
[null,null,null,38886,16345,"0_Sun Dec 29 2024 11:13:29 GMT+0800","2024-12-02T23:59:35","Observation","Owner / Marine / Tech. Suptd.","ISM Audit","LOOSE HEAVY ITEMS IN STEERING GEAR (ROPE STORE) and NEXT TO DG 1/ HYDROPHORE) ARE NOT SECURED.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Human Error","","","","","BEFORE DEPARTURE ALL LOOSE HEAVY ITEMS IN STEERING GEAR (ROPE STORE) and NEXT TO DG 1/ HYDROPHORE) SECURED AND LASHED","2025-03-01T23:59:35","","Completed","2024-12-05T23:59:35","No","No","No","Internal"]
[null,null,null,38887,50623,"0_Sun Dec 29 2024 11:04:07 GMT+0800","2024-12-02T23:59:35","Observation","Owner / Marine / Tech. Suptd.","ISM Audit","LO MSDS (SDS) ARE OLDER THAN 5 YEARS; TO BE REPLACED WITH LATEST VERSIONS. THIS INCLUDES FOR CHEMICALS TOO","Documentation","Cert. & Docu.","Inappropriate Procedure","","","","","LO, CHEMICAL MSDS  REPLACED WITH LATEST VERSIONS.","2025-03-01T23:59:35","","Completed","2024-12-05T23:59:35","No","No","No","Internal"]
[null,null,null,38889,34542,"50_Sun Dec 29 2024 10:57:57 GMT+0800","2024-12-02T23:59:35","Observation","Owner / Marine / Tech. Suptd.","ISM Audit","STEERING FLAT PATHWAY AROUND THE STEERING GEAR IS SLIPPERY (PAINTED OVER ANTI SKID GRIT)","Miscellaneous","Eng. / Strg. Comp.","Inappropriate Procedure","","","","","STEERING FLAT PATHWAY AROUND THE STEERING GEAR TO BE PAINTED WITH ANTI SKID GRIT","2025-02-28T23:59:35","","Completed","2025-01-10T23:59:35","No","No","No","Internal"]
[null,null,null,38899,24182,"50_Sun Dec 29 2024 13:13:34 GMT+0800","2024-12-05T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Emergency switch board control relays to be renewed-5yearly job","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.16","Very High","","","Carried out renewal of over current relay,Under voltage relay,auxiliary relays(E52X1,E52CX,E84U).6 nos auxiliary relays are remaining to be renewed. To carry out the renewal,the emergency switchboard requires isolation.To be carried out at anchorage at a suitable opportunity,","2025-01-31T23:59:35","","Completed","2025-01-18T23:59:35","No","No","No","Internal"]
[null,null,null,38901,14063,"50_Mon Dec 30 2024 14:46:04 GMT+0800","2024-12-11T23:59:35","Observation","Ship Staff","Ship Staff Insp.","SOX/NOX RATIO SHOWING INCORRECT IN EGCS CEMS AND HMI PANEL","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.11","Medium","","","LOG FILES TO BE SENT TO THE MAKER FOR INVESTIGATION.THERE IS SOFTWARE ISSUE IN TRANSFERRING THE LOG FILES FROM CEMS PANEL TO THE DESIGNATED LAPTOP DUE TO PROGREAM ERROR.OFFICE CORRESPONDENCE IS IN PROGRESS.SOX /NOX RATIO IS CALCULATED MANUALLY AT PRESENT ON DAILY BASIS.\nSE TO BE ATTAENDED FOR TROUBLESHOOTING.","2025-03-31T23:59:35","","Completed","2025-02-06T23:59:35","No","No","No","Internal"]
[null,null,null,38904,17411,"50_Thu Dec 26 2024 23:50:24 GMT+0800","2024-12-11T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Stbd Hose handling crane runner wire has a delay of 6 sec  during operation","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.50","Medium","","","Limit switch renewed","2025-03-09T23:59:35","","Completed","2024-12-26T23:59:35","No","No","No","Internal"]
[null,null,null,38894,97947,"50_Sun Dec 22 2024 14:19:22 GMT+0800","2024-12-12T23:59:35","Observation","Ship Staff","Ship Staff Insp.","LO Purifier no:2 Heater needs to be cleaned as temperature is not rising effectively.","E/R - Purifier","Eng. / Strg. Comp.","Equipment Related","","","","","Heater cleaning  carried out.","2025-01-31T23:59:35","","Completed","2024-12-27T23:59:35","No","No","No","Internal"]
[null,null,null,38897,28900,"50_Thu Dec 26 2024 23:13:53 GMT+0800","2024-12-18T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Stripper pneumatic controller from CCR is not operational. Stripper pump strokes has to be controlled from Pump room locally.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.8","Medium","","","to investigate and rectify","2025-01-21T23:59:35","","Completed","2025-01-13T23:59:35","No","No","No","Internal"]
[null,null,null,38906,77760,"50_Thu Dec 26 2024 23:07:18 GMT+0800","2024-12-20T23:59:35","Observation","Ship Staff","Ship Staff Insp.","TRO NO.1 S/F alarms is coming on BWTS computer. TRO No.1 is unavailable to use due to the alarm during BWTS use.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","6.21","High","","","Cleaned the inlet control air section filter and found in good order.","2025-03-31T23:59:35","","Completed","2025-02-10T23:59:35","No","No","No","Internal"]
[null,null,null,38892,23243,"50_Thu Dec 26 2024 23:08:37 GMT+0800","2024-12-21T23:59:35","Observation","Ship Staff","Ship Staff Insp.","1 number Personal gas meter GX 2009 S. no. 741080277Rn showing FAIL 021 alarm.","Miscellaneous","Safety / LSA / FFA","Equipment Related","6.21","High","","","Office informed, gas meter taken out of service, vessel have 5 personal gas meters and complying with SMS","2025-03-19T23:59:35","","Completed","2025-01-09T23:59:35","No","No","No","Internal"]
[null,null,null,38896,90408,"50_Thu Dec 26 2024 23:57:53 GMT+0800","2024-12-23T23:59:35","Observation","Ship Staff","Ship Staff Insp.","C Deck Weather tight door damaged from the hinges. Door has dropped in height","Miscellaneous","General Appearance","Equipment Related","11.6","Medium","","","Hinges renewed, door fixed properly.","2025-03-31T23:59:35","","Completed","2025-01-21T23:59:35","No","No","No","Internal"]
[null,null,null,38893,79845,"50_Fri Jan 03 2025 20:51:46 GMT+0800","2025-01-02T23:59:35","Observation","Ship Staff","Ship Staff Insp.","In pump room,Deck seal Overboard line section observed to have pin hole leaks","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.27","Medium","","","Line renewed","2025-04-02T23:59:35","","Completed","2025-01-08T23:59:35","No","No","No","Internal"]
[null,null,null,38909,95533,"50_Thu Jan 02 2025 20:49:46 GMT+0800","2025-01-02T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Air valve for carrying out Exxon test of Cargo sea chest valve is missing wheel. Valve is frozen in place.  Inlet air valve cannot be operated","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","Air valve renewed. Pressure regulator found choked. Line cleared, new regulator installed. Sea chest testing carried out satisfactorily","2025-01-31T23:59:35","","Completed","2025-01-03T23:59:35","No","No","No","Internal"]
[null,null,null,38903,56640,"50_Wed Jan 08 2025 16:42:06 GMT+0800","2025-01-04T23:59:35","Defect,Observation","Ship Staff","Ship Staff Insp.","On deck,4 set of bunker  tanks vent heads to be repaired for covers.","Deck - Pipe / Fittings","General Appearance","Equipment Related,External Factors,Human Error","6.7","High","","","All the vent head to be de-rusted & cleaned, if reqd then fabricate a new for damage portion. Vessel will send a sheet for vent head renewal including dimension.","2025-04-04T23:59:35","","Completed","2025-02-12T23:59:35","No","No","No","Internal"]
[null,null,null,38900,17614,"50_Mon Jan 06 2025 14:03:36 GMT+0800","2025-01-05T23:59:35","Defect,Observation","Ship Staff","Ship Staff Insp.","LSMGO Settling tank outlet QCV valve is leaking for Oil through gland.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related,Human Error,Industry Issue","10.32","Very High","","","Tank to be lowered at below suction low level and removed the bonnet cover and rectify the leak.","2025-04-05T23:59:35","","Completed","2025-01-31T23:59:35","No","No","No","Internal"]
[null,null,null,38895,78393,"50_Mon Jan 13 2025 01:36:34 GMT+0800","2025-01-13T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Hydraulic leak from brake cylinder of M1 winch","Deck - Mooring Machinery","Mooring","Equipment Related","","","","","Leak rectified","2025-04-12T23:59:35","","Completed","2025-01-17T23:59:35","No","No","No","Internal"]
[null,null,null,38898,86517,"0_Mon Jan 13 2025 01:43:53 GMT+0800","2025-01-13T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Drains in spare cabins and around accommodation are chocked.","Miscellaneous","General Appearance","Human Error","","","","","Drains cleared","2025-04-12T23:59:35","","Completed","2025-01-30T23:59:35","No","No","No","Internal"]
[null,null,null,38905,38326,"50_Mon Jan 13 2025 01:47:12 GMT+0800","2025-01-13T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Various dimmers for lights and lamp test buttons for various panels on bridge inoperational ","Navigation - Others","Navigation","Equipment Related","","","","","Troubleshooting carried out, all in order now.","2025-04-12T23:59:35","","Completed","2025-02-09T23:59:35","No","No","No","Internal"]
[null,null,null,38907,42449,"50_Wed Jan 22 2025 15:11:36 GMT+0800","2025-01-18T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Oxy/Acetylene Hoses are not secured with ear clamps","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related,External Factors,Human Error","10.32","Very High","","","To be secured with Ear clamps,RO will raise in Store.","2025-04-18T23:59:35","","Completed","2025-02-12T23:59:35","No","No","No","Internal"]
[null,null,null,38902,73224,"50_Tue Jan 21 2025 15:58:17 GMT+0800","2025-01-20T23:59:35","Defect,Observation","Ship Staff","Ship Staff Insp.","Low expansion deck foam pump is leaking through mechanical seal for liquid.","Critical Equip.","Eng. / Strg. Comp.","Equipment Related,External Factors,Human Error","5.35","Medium","","","Deck Foam Pump to be overhauled.,","2025-04-21T23:59:35","","Completed","2025-02-06T23:59:35","No","No","No","Internal"]
[null,null,null,null,28211,"50_Sun Sep 29 2024 04:32:11 GMT+0800","2024-06-15T08:00:00","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Mooring winch gear units to derust","Deck - Mooring Machinery","ISM Related","Equipment Related","","","","","Mooring winch gear units  derusting completed","2025-03-31T08:00:00","","Completed","2025-02-24T08:00:00","No","No","No","Internal"]
[null,null,null,null,37570,"50_Sun Sep 29 2024 04:26:49 GMT+0800","2024-06-15T08:00:00","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Numerous Mooring winches require derust and upgradation","Deck - Mooring Machinery","ISM Related","Equipment Related","","","","","Numerous Mooring winches require derusting and painting completed","2025-03-31T08:00:00","","Completed","2025-02-24T08:00:00","No","No","No","Internal"]
[null,null,null,null,65112,"50_Wed Jun 26 2024 23:04:49 GMT+0800","2024-06-25T08:00:00","Observation","Ship Staff","Ship Staff Insp.","During routine maintenance on the aft vapor manifold on port side, the drain pipe got pin hole.","Deck - Pipe / Fittings","Cargo / Ballast Systems","External Factors","","","","","Cold work carried out to stop the leak.\nJob entered in refman","2025-03-31T08:00:00","DPEO240175","Completed","2025-02-24T08:00:00","No","No","Yes","Internal"]
[null,null,null,null,44753,"50_Tue Dec 03 2024 11:55:52 GMT+0800","2024-12-03T08:00:00","Observation","Ship Staff","Ship Staff Insp.","4 C COT Vapour pressure sensor erratic, with many times pressure value not showing","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.19","High","","","Connections found broken, new connections made with connectors, now in order.","2025-03-31T08:00:00","","Completed","2025-02-14T08:00:00","No","No","No","Internal","RO not visible. MAke RO in 2025."]
[null,null,null,null,59312,"50_Thu Dec 26 2024 23:47:45 GMT+0800","2024-12-18T08:00:00","Observation","Ship Staff","Ship Staff Insp.","3P COT main valve CAV176, Valve indication is erratic","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.11","Medium","","","Switch changed, now working satisfactorily.","2025-03-31T08:00:00","DPEO250065","Completed","2025-02-20T08:00:00","No","No","No","Internal","Spares on order."]
[null,null,null,null,62290,"50_Mon Jan 06 2025 20:53:40 GMT+0800","2025-01-05T08:00:00","Defect,Observation","Ship Staff","Ship Staff Insp.","In P/Room,Main ballast system both pump suction filter is bypass due to high filter DP Alarm, filter elements to be cleaned and check the proxy sensors for malfunctioning.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related,External Factors,Human Error,Inappropriate Procedure","6.21","High","","","Both Filters candles cleaned. will check operation of the system during ballasting operation","2025-04-05T08:00:00","","Completed","2025-02-21T08:00:00","No","No","No","Internal","We will be arranging maker for NF upgrade next call Singapore."]
[null,null,null,null,64432,"0_Mon Jan 13 2025 01:41:43 GMT+0800","2025-01-13T08:00:00","Observation","Ship Staff","Ship Staff Insp.","PV Breaker gauge glass unit requires overhaul","Deck - Pipe / Fittings","Cargo / Ballast Systems","External Factors","","","","","Gauge cock freed","2025-04-12T08:00:00","","Completed","2025-02-18T08:00:00","No","No","No","Internal","Why waiting for this job? Will not take much time to complete"]
[null,null,null,null,71408,"50_Thu Jan 16 2025 17:44:12 GMT+0800","2025-01-16T08:00:00","Observation","Ship Staff","Ship Staff Insp.","No.3 COP mechanical seal leak alarm erratic during testing","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","Connecter renewed, now working satisfactorily","2025-03-28T08:00:00","","Completed","2025-02-11T08:00:00","No","No","No","Internal","What was outcome of troubleshooting."]
[null,null,null,null,27862,"50_Fri Jan 17 2025 20:56:56 GMT+0800","2025-01-16T08:00:00","Observation","Ship Staff","Ship Staff Insp.","leak from M1 mooring winch brake cylider shaft seal","Deck - Mooring Machinery","Mooring","Equipment Related","9.14","Medium","","","Seals renewed.","2025-03-31T08:00:00","DPEO250086","Completed","2025-02-22T08:00:00","No","No","No","Internal","Will supply spares once available."]
[null,null,null,null,57622,"50_Wed Jan 22 2025 17:59:57 GMT+0800","2025-01-21T08:00:00","Observation","Ship Staff","Ship Staff Insp.","Safety walkway few stanchions supports are wasted due to which complete rigging of walkway cannot be done.","Miscellaneous","General Appearance","External Factors","","","","","Wire ropes put in place with accessories where stanchions cannot be put in place, Job added in refman for stanchions support repairs.","2025-04-21T08:00:00","","Completed","2025-02-11T08:00:00","No","No","No","Internal","Can it be repaired without hotwork?"]
[null,null,null,null,82339,"50_Sat Jun 17 2023 20:29:01 GMT+0800","2023-05-26T08:00:00","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","On main deck cable tray plate corroded at many places. Same to repair","Deck - Pipe / Fittings","General Appearance","External Factors","11.5","Medium","","","Hot work repairs/renewal is required, job added in refman","2025-03-31T08:00:00","","Completed","2025-02-24T08:00:00","No","No","No","Internal"]
[null,null,null,null,83242,"50_Tue Mar 26 2024 17:33:09 GMT+0800","2024-03-07T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Stbd Bridge wing RPM Indicator(Newly Installed) not in sync with main bridge RPM indicator","Navigation - Others","Navigation","Equipment Related","","","","","Currently the indicator is having a difference of just 1 RPM, will continue to monitor.","2025-03-28T08:00:00","","Completed","2025-02-01T08:00:00","No","No","Yes","Internal"]
[null,null,null,null,42565,"50_Sat Feb 24 2024 17:20:03 GMT+0800","2024-05-30T08:00:00","Observation","Ship Staff","Ship Staff Insp.","Stbd windlass found wobbling during operation","Deck - Mooring Machinery","Mooring","Equipment Related","9.20","Medium","","","Split bearings inspected for the port side warping drum side , bush found broken .  always keep it highly greased , nipples to be clean & clear , correspondence in progress.Wobbling checked in presence of superitendent and found within limits. Job deffered to dry dock as per instructions from office.","2025-03-31T08:00:00","","Completed","2024-12-01T08:00:00","No","No","Yes","Internal","To be attended next opportunity."]
[null,null,null,null,42986,"50_Wed Jun 26 2024 23:09:09 GMT+0800","2024-06-21T08:00:00","Observation","Ship Staff","Ship Staff Insp.","The SAAB RADAR dome supports found to be in very bas state after carrying out maintenance.","","Cargo / Ballast Systems","External Factors","","","","","Job entered in refman.","2025-03-31T08:00:00","","Completed","2025-02-24T08:00:00","No","No","Yes","Internal"]
[null,null,null,null,66260,"50_Wed Jun 26 2024 23:08:02 GMT+0800","2024-06-24T08:00:00","Observation","Ship Staff","Ship Staff Insp.","The manifold drip tray was found to be leaking and when investigated found that the drip has a crack at the bottom.","","Cargo / Ballast Systems","External Factors","","","","","Cold work carried out. To renew during DD, Job entered in refman","2025-03-31T08:00:00","","Completed","2025-02-24T08:00:00","No","No","Yes","Internal"]
[null,null,null,null,39989,"50_Wed Jun 26 2024 23:06:32 GMT+0800","2024-06-24T08:00:00","Observation","Ship Staff","Ship Staff Insp.","The steam line to deck seal was found to be leaking near the break of accommodation. The pipe is penetrating through the deck into the pump room .","","Cargo / Ballast Systems","External Factors","","","","","Cold work carried out and leak arrested.\nTo crop and renew at next opportunity. (Or during DD), Job entered in Refman","2025-03-31T08:00:00","","Completed","2025-02-24T08:00:00","No","No","Yes","Internal"]
[null,null,null,null,56357,"50_Mon Jan 13 2025 21:16:51 GMT+0800","2025-01-13T08:00:00","Defect,Observation,Critical Equipment","Ship Staff","Ship Staff Insp.","In Stripper steam line,ER steam stripper controller to deck is malfunctioning,","Cargo Mach.,E/R - Boiler","Eng. / Strg. Comp.","Equipment Related,External Factors,Inappropriate Procedure,Human Error","10.32","Very High","","","Controller troubleshooting to be carried out and if reqd then will raise the RO for Spares.","2025-04-13T08:00:00","","Completed","2025-02-03T08:00:00","No","No","No","Internal","No RO no mentioned."]
[null,null,null,null,26198,"50_Mon Jan 06 2025 20:58:42 GMT+0800","2025-01-06T08:00:00","Defect,Observation","Ship Staff","Ship Staff Insp.","On Minerlizer unit soft patch work has been carried out at bottom of the tanks on support brackets.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related,External Factors,Human Error","10.32","Very High","","","Unit to be isolated and transferred to ER Workshop for hot work.","2025-04-06T08:00:00","","Completed","2025-02-21T08:00:00","No","No","No","Internal","When do you plan to repair it?"]
[null,null,null,null,69758,"50_Mon Jan 06 2025 21:00:39 GMT+0800","2025-01-06T08:00:00","Defect","Ship Staff","Ship Staff Insp.","ER Ultrasonic Machine not being used since long.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related,External Factors,Human Error","10.32","Very High","","","Machine to be checked for troubleshooting","2025-04-24T08:00:00","","Completed","2025-02-20T08:00:00","No","No","No","Internal","Revert with troubleshooting outcome."]
[null,null,null,null,41162,"50_Fri Jan 10 2025 17:06:19 GMT+0800","2025-01-04T08:00:00","Defect,Observation","Ship Staff","Ship Staff Insp.","In Veg Room,Refrigerant gas return line is in suspended condition.","Accommodation","MLC Related","Equipment Related,External Factors,Inappropriate Procedure","10.32","Very High","","","Need to be secured the gas line with clamps","2025-04-04T08:00:00","","Completed","2025-02-19T08:00:00","No","No","No","Internal","These small jobs should be fixed immediately and not keep pending for long."]
[null,null,null,null,32387,"50_Sat Jan 11 2025 21:04:32 GMT+0800","2025-01-04T08:00:00","Observation","Ship Staff","Ship Staff Insp.","Around the accomodation and aft poop deck light fixturs base is in rusted condition.","Accommodation,Elect. Mach. & Equip.","General Appearance","Equipment Related,External Factors,Human Error,Inappropriate Procedure","10.32","Very High","","","Corroded base light fixtures to be repaired or renewed.","2025-04-04T08:00:00","","Completed","2025-02-24T08:00:00","No","No","No","Internal"]
[null,null,null,null,26147,"50_Sun Dec 22 2024 13:33:25 GMT+0800","2024-12-04T08:00:00","Observation","Ship Staff","Ship Staff Insp.","The AE 3 save all is leading to the clean drain tank.The same needs to be directed to the waste oil tank.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","New line to be fabricated from the save all leading to waste oil tank.,Job is shifted to refman.","2025-03-31T08:00:00","","Completed","2025-02-24T08:00:00","No","No","No","Internal","Job to be shifted to Refman."]
[null,null,null,null,98506,"0_Sun Dec 29 2024 11:22:03 GMT+0800","2024-12-02T08:00:00","Observation","Owner / Marine / Tech. Suptd.","ISM Audit","SAVE ALL AROUND FW HYDROPHORE & HOTWELL TRAY IS CORRODED AND HOLED.","E/R - Pipes/ valves & fittings","Structural Condn. / WT integrity ","Equipment Related","10.32","Very High","","","In ER All save all tray to be de-rusted and if reqd then re fabricated or repaired.","2025-03-30T08:00:00","","Completed","2025-01-22T08:00:00","No","No","No","Internal"]
[null,null,null,null,66015,"50_Tue Sep 17 2024 07:13:24 GMT+0800","2024-09-04T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Emergency fire pump sea chest valve found not holding","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Defect  recorded in refman for inspection/renewal of the sea chest valve in dry dock.Transferred to Refman.","2025-03-31T08:00:00","","Completed","2025-02-24T08:00:00","No","No","No","Internal"]
[null,null,null,null,11567,"50_Tue Aug 06 2024 08:42:32 GMT+0800","2024-07-15T08:00:00","Defect","Ship Staff","Ship Staff Insp.","2 OF THE BUNKER VALVES ON DECK ARE IN FROZEN CONDITION FOR VERY LONG PAST , THEY HAVE TO BE CHANGED AT SUITIBLE OPPORTUNITY","Deck - Pipe / Fittings","MARPOL Related","External Factors,Human Error,Industry Issue","6.7","High","","","1 HFO and 1 LSMGO bunker line valve renewal will plan it accordingly. Vessel has spare  1 LSMGO  valves and all inline valves are eased up.","2025-03-31T08:00:00","","Completed","2025-02-24T08:00:00","No","No","Yes","Internal","Why pending for so long?"]
[null,null,null,null,63682,"50_Fri May 31 2024 09:58:14 GMT+0800","2024-05-30T08:00:00","Defect","Ship Staff","Ship Staff Insp.","HIGH SEA CHEST OUTBOARD VALVE FOUND NOT HOLDING","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.31","Very High","","","As of now,Filter has been opened and strainer cleaned.but ship side valve is badly leaking for water and suspecting ropes is entangle in valve seat and unable to remove.strainer condition is good.\nDivers to be arranged in suitable port for blanking the ship side and to assess the valve.Transferred to Refman.","2025-03-31T08:00:00","","Completed","2025-02-24T08:00:00","No","No","Yes","Internal"]
[null,null,null,null,84690,"50_Mon Jan 13 2025 02:09:07 GMT+0800","2025-01-13T08:00:00","Observation","Ship Staff","Ship Staff Insp.","Some fire and foam line isolation valves and few foam monitor valves are hard to operate.","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","Isolation and foam monitor valves freed up","2025-04-12T08:00:00","","Completed","2025-02-24T08:00:00","No","No","No","Internal","Has this job not been attended in this long voyage? Overhaul the valves prior discharge port."]
[null,null,null,null,47482,"50_Mon Feb 24 2025 21:55:34 GMT+0800","2025-01-20T08:00:00","Defect","Ship Staff","Ship Staff Insp.","FWD atmospheric condenser is chocked for sea water flow.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related,External Factors,Human Error","10.32","Very High","","","Complete Condenser unit to be renewed.as per office advised will be carried out in DD.","2025-04-19T08:00:00","DPEO250085","Completed","2025-03-01T08:00:00","No","No","No","Internal"]
[null,null,null,null,91239,"50_Mon Feb 24 2025 16:25:51 GMT+0800","2025-02-10T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Auxiliary Engine #1 LO cooler is leaking for LT water and sump LO.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related,External Factors,Inappropriate Procedure","10.32","Very High","","","Brazed type plate cooler to be renewed.","2025-05-10T08:00:00","DPEO250112","Completed","2025-03-03T08:00:00","No","No","No","Internal"]
[null,null,null,null,46820,"50_Mon Feb 24 2025 16:05:32 GMT+0800","2024-12-13T08:00:00","Defect,Observation","Ship Staff","Ship Staff Insp.","In EGCS,WMS-002 unit PAH value is not showing in WMS panel.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","External Factors,Equipment Related,Inappropriate Procedure","10.32","Very High","","","Need to be renewed PAH sensor for due for calibration.As of now PAH value is showing in WMS 002 panel.","2025-04-12T08:00:00","DPEO250024","Completed","2025-03-01T08:00:00","No","No","No","Internal"]
[null,null,null,null,12573,"50_Sun Jan 19 2025 02:40:51 GMT+0800","2025-01-19T08:00:00","Defect,Observation","Ship Staff","Ship Staff Insp.","EGCS CEMS SOX/CO2 Calibration Gas has expired.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related,External Factors,Human Error","10.11","Medium","","","Calibration gas is expired on Dec'24 and Bottle connector is missing.","2025-04-19T08:00:00","DPEO250082","Completed","2025-03-03T08:00:00","No","No","No","Internal","will be connected passing Singapore."]
[null,null,null,null,73593,"50_Thu Jan 16 2025 16:01:14 GMT+0800","2025-01-15T08:00:00","Defect,Observation","Ship Staff","Ship Staff Insp.","ECR #1 AC unit compressor is malfunctioning due to low insulation.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related,External Factors,Human Error","10.32","Very High","","","Complete hermetic compressor unit to be renewed & evaporator is swapped to ECR #2 unit. so both compressor and evaporator to be renewed for ECR #1 AC.","2025-04-15T08:00:00","DPEO250076","Completed","2025-03-03T08:00:00","No","No","No","Internal","Spares on order."]
[null,null,null,null,95197,"50_Thu Jan 16 2025 19:18:24 GMT+0800","2025-01-16T08:00:00","Defect","Ship Staff","Ship Staff Insp.","The bottom section tubes of the ER FWD Atmospheric Condenser are clogged with hard rock salt.","E/R - Boiler,E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related,External Factors,Human Error","10.32","Very High","","","Complete unit to be off-landed for shore servicing or to be received new condenser.As per office advised will be carried out in next scehdule DD.","2025-04-16T08:00:00","DPEO250085","Completed","2025-03-01T08:00:00","No","No","No","Internal","Awaiting for quote."]
[null,null,null,null,34867,"50_Wed Jan 15 2025 16:02:38 GMT+0800","2025-01-11T08:00:00","Observation","Ship Staff","Ship Staff Insp.","ER Cargo oil pump turbine all 3 auto grease cup is in broken condition","Cargo Mach.","Cargo / Ballast Systems","Equipment Related,External Factors,Human Error","","","","","All 3 Auto grease cup to be renewed.","2025-04-11T08:00:00","DPEO250074","Completed","2025-03-03T08:00:00","No","No","No","Internal","Spares on order."]
[null,null,null,null,72341,"50_Sun Dec 22 2024 14:50:47 GMT+0800","2024-12-12T08:00:00","Observation","Ship Staff","Ship Staff Insp.","AE# 3 Autofilter solenoid valve is leaking for air.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Presently the autofilter is working in auto.However the solenoid valve needs to be renewed.Ship staff will place an RO for the same in january 2025.\nWe have removed and cleaned the valve but still is leaking.","2025-03-31T08:00:00","DPEO250001","Completed","2025-03-03T08:00:00","No","No","No","Internal","Spares on order."]
[null,null,null,null,13557,"50_Tue Sep 03 2024 08:00:20 GMT+0800","2024-08-20T08:00:00","Defect","Ship Staff","Ship Staff Insp.","RPLS servo pp no:2 pressure switch faulty.","E/R - Aux. Mach.,E/R - Main Engine","","Equipment Related,External Factors,Inappropriate Procedure","10.32","Very High","","","Pressure Switch to be renewed.","2025-03-31T08:00:00","DPEO250039","Completed","2025-03-03T08:00:00","No","No","No","Internal"]
[null,null,null,null,16131,"0_Mon Jul 15 2024 23:32:56 GMT+0800","2024-07-05T08:00:00","Observation","Ship Staff","Ship Staff Insp.","The loadicator computer hanging everyday.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","New loadicator received","2025-03-31T08:00:00","DPEO245082","Completed","2025-03-03T08:00:00","No","No","Yes","Internal"]
[null,null,null,null,58012,"50_Wed Jan 08 2025 16:06:12 GMT+0800","2025-01-07T08:00:00","Defect,Observation","Ship Staff","Ship Staff Insp.","In ME RPLS Unit,Duplex filter unit changeover cock gland is leaking for cylinder oil.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related,External Factors,Human Error,Industry Issue","10.32","Very High","","","Changeover cock seal rings to be overhauled.","2025-04-07T08:00:00","DPEO250051","Completed","2025-03-04T08:00:00","No","No","No","Internal","Waiting for quote"]
[null,null,null,null,97687,"50_Wed Nov 13 2024 11:35:09 GMT+0800","2024-11-12T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Waste oil incinerator burner no:2 ignition transformer faulty","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","RO placed for a spare transformer","2025-03-11T08:00:00","DPEO250010","Completed","2025-03-04T08:00:00","No","No","No","Internal","Spares on order."]
[null,null,null,null,88561,"50_Wed Jan 08 2025 16:13:13 GMT+0800","2025-01-08T08:00:00","Defect,Observation","Ship Staff","Ship Staff Insp.","In Galley,2 set of hot plates to be renewed for bulge and crack condition.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related,External Factors,Human Error,Inappropriate Procedure","11.13","Low","","","2 Set of hot plate observed bulge and in crack state,giving low insulation alarm.","2025-04-08T08:00:00","DPEO250046","Completed","2025-03-04T08:00:00","No","No","No","Internal","Spares on order, will be connected next call."]
[null,null,null,null,29150,"50_Wed Jan 08 2025 16:34:42 GMT+0800","2025-01-07T08:00:00","Defect,Observation","Ship Staff","Ship Staff Insp.","In ME Local Maneuvering platform, Fuel Oil pressure gauge is defective.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related,External Factors,Inappropriate Procedure","10.33","High","","","Pressure gauge to be renewed with spare OEM one.","2025-04-07T08:00:00","DPEO250063","Completed","2025-03-04T08:00:00","No","No","No","Internal","Spare on order."]
[null,null,null,null,11896,"50_Thu Jan 09 2025 23:58:23 GMT+0800","2025-01-03T08:00:00","Defect,Observation","Ship Staff","Ship Staff Insp.","Observed in No 1 Main Air compressor that oil filter cap was found broken and repaired with cold patch work.","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related,External Factors,Human Error","10.32","Very High","","","Waiting for Spares to carry out permanent repair , Raised PO for the same .","2025-04-03T08:00:00","DPEO250023","Completed","2025-03-04T08:00:00","No","No","No","Internal","Spares on order."]
[null,null,null,null,17691,"50_Thu Jan 09 2025 23:40:32 GMT+0800","2025-01-02T08:00:00","Defect,Observation","Ship Staff","Ship Staff Insp.","Observed HFO Purifier #2 air valve block is leaking,  As the spring loaded screw in Air valve block was found missing","E/R - Purifier","Eng. / Strg. Comp.","Equipment Related,External Factors,Human Error","10.32","Very High","","","Air valve block need to renewed, for starting this pfr we need to shift  #1 pfr air block .","2025-04-02T08:00:00","DPEO250048","Completed","2025-03-03T08:00:00","No","No","No","Internal","Spares on order."]
[null,null,null,null,14652,"50_Sat Jan 11 2025 21:01:41 GMT+0800","2025-01-04T08:00:00","Critical Equipment,Defect,Observation","Ship Staff","Ship Staff Insp.","Both Deck seal pump performance is poor.","E/R - Pumps,Cargo Mach.","Eng. / Strg. Comp.","Equipment Related,Human Error,External Factors","10.32","Very High","","","Both deck seal pump to be overhauled.","2025-04-04T08:00:00","DPEO250004/6","Completed","2025-03-04T08:00:00","No","No","No","Internal","Spares on order."]
[null,null,null,null,58512,"50_Mon Feb 24 2025 17:07:01 GMT+0800","2025-02-17T08:00:00","Defect","Ship Staff","Ship Staff Insp.","EGCS SW pump VFD installation on panel.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related,External Factors,Inappropriate Procedure","10.32","Very High","","","Portable cabinet AC to be installed on VFD units.","2025-05-17T08:00:00","DPEO250120","Completed","2025-03-04T08:00:00","No","No","No","Internal"]
[null,null,null,null,41821,"50_Wed Feb 12 2025 16:06:07 GMT+0800","2025-02-04T08:00:00","Defect","Ship Staff","Ship Staff Insp.","LT Pump #1 to be overhauled for new shaft and shaft seal.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related,External Factors,Human Error","10.32","Very High","","","LT Pump #1 was leaking from shaft seal and pump is overhauled with new make shift arrangement shaft seal,. Found impeller shaft and nut is in tag weld condition,As of now,pump assembled and in use but slightly leaking from seal.","2025-03-15T08:00:00","DPEO250105","Completed","2025-03-04T08:00:00","No","No","No","Internal","Spares on order."]
[null,null,null,null,13034,"50_05/07/2020 4:44:55 AM","2020-06-10T08:00:00","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","EGCS sea water chest suction valve remote operating unit, no dates of last tried out .\n\n","Miscellaneous","Cert. & Docu.","Human Error","10.12","Very High","","","EGCS sea water chest suction valve remote operating unit-JOB INCLUDED IN PMS,tred out on 17-July-2020.\n\n\n\n","2020-08-10T08:00:00","","Completed","2020-07-12T08:00:00","No","No","No","Internal"]
[null,null,null,null,64557,"50_Mon Jan 06 2025 20:51:49 GMT+0800","2025-01-05T08:00:00","Defect,Observation","Ship Staff","Ship Staff Insp.","In IG System,#2 Blower Ampere meter is out of order.","Cargo Mach.,Inert Gas","Cargo / Ballast Systems","Equipment Related,External Factors,Human Error","8.3","Very High","","","IG Blowers # 2 tried out for a few minutes, but EOCR converter is out of operation for ampere meter.","2025-04-05T08:00:00","DPEO250069","Completed","2025-03-04T08:00:00","No","No","No","Internal"]
[null,null,null,null,99644,"50_Sat Jan 11 2025 20:49:28 GMT+0800","2025-01-11T08:00:00","Observation,Defect","Ship Staff","Ship Staff Insp.","LSMGO Boiler #2 Pump is leaking for Oil through mechanical seal.","E/R - Boiler,E/R - Pumps","Eng. / Strg. Comp.","Equipment Related,External Factors,Inappropriate Procedure","10.32","Very High","","","Pump to be overhauled.,Vessel does not have any spares for the pump and pump is in working condition but slight leakages from the mech seal is observed.","2025-04-11T08:00:00","DPEO250071","Completed","2025-03-06T08:00:00","No","No","No","Internal","Does vessel not have seal for renewal?"]
[null,null,null,null,90037,"0_Sat Aug 19 2023 11:56:44 GMT+0800","2023-08-01T08:00:00","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","COW Line having thick rust spots","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","11.1","High","","","Derusting and painting of major rust spots carried out.","2025-03-31T08:00:00","","Completed","2025-03-05T08:00:00","No","No","No","Internal"]
[null,null,null,null,79107,"50_Sat Mar 08 2025 08:40:23 GMT+0800","2025-02-01T08:00:00","Observation","Ship Staff","Ship Staff Insp.","Autopilot unit showing \"caution\" and \"indicate\" alert, error code is for memory full. Autopilot is functioning properly.","Navigation - Others","Navigation","Equipment Related","","","","","Technician attended the vessel at HuangDao and rectified the issue.","2025-04-30T08:00:00","DPEO250027","Completed","2025-03-12T08:00:00","No","No","No","Internal"]
[null,null,null,null,72948,"50_Sun Jan 19 2025 21:47:29 GMT+0800","2025-01-19T08:00:00","Critical Equipment,Defect,Observation","Ship Staff","Ship Staff Insp.","ME LT Pump #1 and #2 are not in stby mode.","Critical Equip.,Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related,External Factors,Human Error","10.32","Very High","","","Technician attended at dailan,china on 16/03/2025.\nsome of the parameter were found wrong, same changed by terasaki technician. presently LT pumps are in Auto, working satisfactory.\n","2025-04-19T08:00:00","","Completed","2025-03-16T08:00:00","No","No","No","Internal",""]
[null,null,null,null,68354,"50_Mon Feb 24 2025 21:57:57 GMT+0800","2025-01-10T08:00:00","Defect,Observation","Ship Staff","Ship Staff Insp.","Shaft Earthing Device millivolt meter unit is malfunctioning","Elect. Mach. & Equip.,E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related,External Factors,Human Error","10.32","Very High","","","Ammeter changed with newly received spare.\nAlso 1 set(3pcs) of brushes renewed, panel lock found damaged same has been changed. found good in order.\n\n","2025-04-09T08:00:00","DPEO250062","Completed","2025-03-18T08:00:00","No","No","No","Internal"]
[null,null,null,null,25896,"50_Thu Jan 23 2025 00:50:53 GMT+0800","2025-01-22T08:00:00","Defect,Observation","Ship Staff","Ship Staff Insp.","INTEMITTENT DISPLAY ISSUE ON ECR CCTV System","Elect. Mach. & Equip.","ISPS Related","Equipment Related,External Factors,Industry Issue","7.12","High","","","Technician attended the issue at singapore. changed master cabin NVR with new and replaced with master NVR in ECR. All camers and display working satisfcatory.","2025-04-22T08:00:00","","Completed","2025-03-27T08:00:00","No","No","No","Internal","Follow up with Auto Elec group."]
[null,null,null,null,99993,"50_Tue Jan 21 2025 19:10:07 GMT+0800","2025-01-21T08:00:00","Critical Equipment,Observation","Ship Staff","Ship Staff Insp.","Oil mist detector ECR Mk6 display showing \"Replace EEPROM\"","E/R - Main Engine,Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related,External Factors,Inappropriate Procedure","10.21","Medium","","","Technician attended the issue at singapore. OMD unit control card renewed with upgraded card. and 6 nos sensors renewed witth new upgraded detectors. All alarms and slowdown tried out. working satisfactory.","2025-04-21T08:00:00","","Completed","2025-03-27T08:00:00","No","No","No","Internal","Follow up with Auto elec group."]
[null,null,null,null,56613,"50_Wed Apr 02 2025 11:04:05 GMT+0800","2025-03-03T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Purifier Room Exhaust Fan Not Working Due to Motor Failure","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","PO received in Singapore 27-Mar-2025 new El motor installed and tested, found working in good condition.","2025-04-30T08:00:00","DPEO250180","Completed","2025-04-02T08:00:00","No","No","No","Internal"]
[null,null,null,null,97721,"0_Mon Jan 13 2025 01:38:44 GMT+0800","2025-01-13T08:00:00","Observation","Ship Staff","Ship Staff Insp.","No. 2 ECDIS monitor performance has deteriorated, same requires renewal. ","","Navigation","Equipment Related","","","","","Service Engineers attended the issue in Singapore and changed the parameter setting as per Service Manual. Now the ECDIS is working in good order.","2025-04-12T08:00:00","DPEO250056","Completed","2025-03-27T08:00:00","No","No","No","Internal"]
[null,null,null,null,98664,"50_Sat Jan 11 2025 20:52:55 GMT+0800","2025-01-11T08:00:00","Critical Equipment,Defect,Observation","Ship Staff","Ship Staff Insp.","During overhauling of OWS pump, observed shaft has heavy pitting marks on the gland packing area & shaft to be renewed.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related,External Factors,Inappropriate Procedure","10.32","Very High","","","Pump was overhauled with available spares and working satisfactory. PO for new spares were received in Singapore.","2025-04-11T08:00:00","DPEO250072","Completed","2025-03-27T08:00:00","No","No","No","Internal","Spares on order."]
[null,null,null,null,85595,"50_Thu Mar 13 2025 17:32:11 GMT+0800","2025-03-13T08:00:00","Defect","Ship Staff","Ship Staff Insp.","COPT #2,Inlet globe valve DN25,200 valve is malfunctioning.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related,External Factors,Inappropriate Procedure","10.32","Very High","","","Valve bonnet was dismantled and disc to aligned with valve stem, found old brass shims pieces got caught between the valve gland and the spindle which prevented the valve to turn. Removed the old shims and replace it with welded collar to avoid overrun of the valve spindle. Box-back the valve and tested, found all working satisfactory.","2025-06-13T08:00:00","","Completed","2025-03-25T08:00:00","No","No","No","Internal"]
[null,null,null,null,77493,"50_Fri Jan 10 2025 01:52:46 GMT+0800","2025-01-09T08:00:00","Defect,Observation","Ship Staff","Ship Staff Insp.","AE#1 & #2 Common JCW preheater is not operational due to Low insulation alarm.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related,External Factors,Human Error","10.32","Very High","","","Pre-heater heating element 2 sets renewed with new spare. control thermostat, safety thermostat and control transformer changed with spare. chamber cleaned. system working in good order.","2025-04-09T08:00:00","DPEO250049","Completed","2025-04-02T08:00:00","No","No","No","Internal",""]
[null,null,null,null,37438,"0_Sun Dec 29 2024 11:24:45 GMT+0800","2024-12-02T08:00:00","Observation","Owner / Marine / Tech. Suptd.","ISM Audit","VARIOUS THERMAL INSULATION IN THE ENGINE ROOM MISSING OR DAMAGED","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Missing and damage section of lagging renewal of this insulation material done on most of the  major equipments .","2025-03-31T08:00:00","DPEO250099","Completed","2025-04-02T08:00:00","No","No","No","Internal"]
[null,null,null,null,78514,"50_Fri Jul 26 2024 00:41:38 GMT+0800","2024-07-09T08:00:00","Defect","Ship Staff","Ship Staff Insp.","1C COT IG branch valve spindle rotating freely.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","","","","","1C COT IG branch valve spindle is rotating freely. the valve is stuck in open position. Valve needs to be renewed, New valves received on 02 Mar 25, will install them after completion of discharging ops in china.\n\n1C IG branch valve renewed","2025-03-31T08:00:00","DPEO240207","Completed","2025-04-04T08:00:00","No","No","Yes","Internal","What is RO  number."]
[null,null,null,null,71568,"50_Tue Mar 11 2025 11:09:16 GMT+0800","2025-03-10T08:00:00","Observation,Critical Equipment","Ship Staff","Ship Staff Insp.","IG O2 Analyzer #1 Unit is Malfunctioning.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related,External Factors","8.11","Medium","","","O2 Analyzer Unit controller renewed completely and calibration carried out as per maker's instruction manual - Span: 20.9 (Instrument Air) / Zero: 1.0% O2 - 99% N2.","2025-06-10T08:00:00","DPEO250151","Completed","2025-04-03T08:00:00","No","No","No","Internal"]
[null,null,null,null,38043,"50_Tue Jan 21 2025 15:59:44 GMT+0800","2025-01-21T08:00:00","Observation","Ship Staff","Ship Staff Insp.","GMDSS station emergency light inoperational.","Navigation - GMDSS & Communication","Navigation","Equipment Related","","","","","DPEO250087 raised for new light.\nNew spare light fitted, Working satisfactorily.","2025-04-20T08:00:00","","Completed","2025-03-05T08:00:00","No","No","No","Internal","Will be connected at next opportunity."]
[null,null,null,null,72882,"50_Mon Jan 06 2025 14:35:46 GMT+0800","2025-01-04T08:00:00","Critical Equipment,Defect,Observation","Ship Staff","Ship Staff Insp.","EGB circulating Pump #1 is leaking for condensate water through seal.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related,External Factors,Inappropriate Procedure,Human Error","10.32","Very High","","","Pump  overhauled , mechanical seal change  and run tested found working satisfactory . and put in service.","2025-04-08T08:00:00","DPEO250053","Completed","2025-04-08T08:00:00","No","No","No","Internal","Spares on order."]
[null,null,null,null,83451,"50_Mon Jan 06 2025 14:22:18 GMT+0800","2025-01-03T08:00:00","Defect,Observation","Ship Staff","Ship Staff Insp.","In AC Compressor unit #1 is not working due to hydraulic relay for unloader unit is malfunctioning.\nBoth Evaporator coil is not maintaining the accomodation temperature.","Accommodation,E/R - Aux. Mach.","MLC Related","Equipment Related,External Factors,Inappropriate Procedure","10.32","Very High","","","AC unit  no.1  unloader unit and evaporator coil checked . and also  conditon of evaporator coil condition inspected ,and  gas leak check found all in normal condition . dryer filter change. and run tested check suction ,discharge and LO pressure found  in normal range , put in used. ","2025-03-24T08:00:00","DPEO250041","Completed","2025-03-24T08:00:00","No","No","No","Internal","Follow up seperately."]
[null,null,null,null,43536,"50_Thu Mar 13 2025 17:29:54 GMT+0800","2025-03-13T08:00:00","Critical Equipment,Defect","Ship Staff","Ship Staff Insp.","Aux Boiler Main Line 1.94Mpa-0.7Mpa Safety valve is leaking for steam.","Cargo Mach.","Eng. / Strg. Comp.","Equipment Related,External Factors,Human Error,Inappropriate Procedure","10.32","Very High","","","Safety valve has been send to shore for reconditioning  same recieved and fitted back. ","2025-06-13T08:00:00","DPEO250153","Completed","2025-04-13T08:00:00","No","No","No","Internal"]
[null,null,null,null,29537,"50_Fri Jan 31 2025 17:09:13 GMT+0800","2025-01-20T08:00:00","Critical Equipment,Defect,Observation","Ship Staff","Ship Staff Insp.","During 3 Monthly ES-A trip,AE # 3 FCU unit is not tripping.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related,External Factors,Human Error","10.32","Very High","","","AE no.3 FCU 1and 2 breaker with the shunt coil renewed.","2025-04-20T08:00:00","DPEO250090","Completed","2025-04-12T08:00:00","No","No","No","Internal","Spares on order."]
[null,null,null,null,13301,"50_Sat Jan 04 2025 19:57:26 GMT+0800","2025-01-04T08:00:00","Defect","Ship Staff","Ship Staff Insp.","IN INERT GAS SYSTEM,BOTH IG BLOWER OUTLET VALVE IN NON-OPERATIVE FOR AUTO OPERATION.","Cargo Mach.,E/R - Aux. Mach.","Cargo / Ballast Systems","Equipment Related,External Factors,Inappropriate Procedure","8.3","Very High","","","Spare received  for both  IG blower outlet valve  solenoid valve and fitted and tried-out found working satisfactory.","2025-04-30T08:00:00","DPEO250019","Completed","2025-04-12T08:00:00","No","No","No","Internal","Spares on order."]
[null,null,null,null,97467,"50_Thu Dec 26 2024 23:41:17 GMT+0800","2024-12-21T08:00:00","Observation","Ship Staff","Ship Staff Insp.","Inlet connector for sample line in No.1 TRO cracked. Repaired by cold work","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","6.21","High","","","spare  filter received and renewed","2025-04-15T08:00:00","DPEO250057","Completed","2025-04-05T08:00:00","No","No","No","Internal","Spares on order."]
[null,null,null,null,88464,"50_Sun Dec 22 2024 14:49:08 GMT+0800","2024-12-05T08:00:00","Defect","Ship Staff","Ship Staff Insp.","FWG high salinity solenoid valve is faulty.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Spares received in Singapore. and fitted and put in used.","2025-04-15T08:00:00","DPEO250013","Completed","2025-04-12T08:00:00","No","No","No","Internal","Spares on order."]
[null,null,null,null,69061,"50_Sun Dec 15 2024 13:50:29 GMT+0800","2024-11-01T08:00:00","Defect","Ship Staff","Ship Staff Insp.","IG fan no:1 and 2 discharge valve solenoids are not working.","Inert Gas","Eng. / Strg. Comp.","Equipment Related","","","","","Spare received  and fitted tried-out found working satisfactory","2025-03-28T08:00:00","DPEO 240261","Completed","2025-04-12T08:00:00","No","No","No","Internal"]
[null,null,null,null,72961,"50_Thu Oct 03 2024 00:34:06 GMT+0800","2024-10-01T08:00:00","Observation","Ship Staff","Ship Staff Insp.","The insulation resistance module on the MSB,ESB,Galley and Forecastle 440 and 220V switchboards need to be renewed as the maximum range of alarm setting is 1.5MOhms. ","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","As per office instructions, the alarm setting in IR module for 440V is 5Mohm and 220V is 2Mohm. RO DPEO250032 and DPEO250033 were cancel as company is about to change the QDMS policy regarding same.","2025-04-30T08:00:00","DPEO 250032,DPEO250033","Completed","2025-03-27T08:00:00","No","No","No","Internal"]
[null,null,null,null,17839,"50_Tue Apr 22 2025 17:06:49 GMT+0800","2025-03-21T08:00:00","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Fwd Fire line pressure gauge to renew","Deck - Pipe / Fittings","Safety / LSA / FFA","Equipment Related","","","","","Pressure gauge renewed","2025-04-10T08:00:00","","Completed","2025-03-23T08:00:00","No","No","No","Internal"]
[null,null,null,null,14138,"50_Tue Apr 22 2025 17:09:05 GMT+0800","2025-03-21T08:00:00","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","All the Drip trays plugs to secure","","Structural Condn. / WT integrity ","Human Error","","","","","Drip tray plugs secured with wire","2025-04-05T08:00:00","","Completed","2025-03-25T08:00:00","No","No","No","Internal"]
[null,null,null,null,67536,"50_Tue Apr 22 2025 16:52:35 GMT+0800","2025-03-21T08:00:00","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Fwd mooring winch gear oil to check pms and renew, if not renewed in recent time","Deck - Mooring Machinery","Mooring","Equipment Related","","","","","Fwd port & stbd Mooring winch oil renewed as per PMS shedule.","2025-05-01T08:00:00","","Completed","2025-12-04T08:00:00","No","No","No","Internal"]
[null,null,null,null,46142,"0_Tue Apr 22 2025 17:18:19 GMT+0800","2025-03-21T08:00:00","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Leaking toilet flush valve to be renewed with new spares","Accommodation","MLC Related","Equipment Related","","","","","Toilet flush valve renewed in upp deck & A- deck common toilet.","2025-03-26T08:00:00","","Completed","2025-03-23T08:00:00","No","No","No","Internal"]
[null,null,null,null,71369,"0_Tue Apr 22 2025 17:13:23 GMT+0800","2025-03-21T08:00:00","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Stbd lifeboat area grating to renew","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","Equipment Related","","","","","Grating renewed at A-Deck stbd side life boat deck","2025-04-05T08:00:00","","Completed","2025-04-02T08:00:00","No","No","No","Internal"]
[null,null,null,null,31957,"0_Tue Apr 22 2025 17:14:55 GMT+0800","2025-03-21T08:00:00","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Gangway last step to renew (stbd)","Deck - Machinery","Safety / LSA / FFA","Equipment Related","","","","","Stbd gangway broken last step to renewed","2025-04-20T08:00:00","","Completed","2025-03-25T08:00:00","No","No","No","Internal"]
[null,null,null,null,68523,"0_Tue Apr 22 2025 17:16:49 GMT+0800","2025-03-21T08:00:00","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Search light bonding wire for both bridge wing to renew","Accommodation","Safety / LSA / FFA","Equipment Related","","","","","Bonding wires in bridge wing renewed. Further inspection of all bonding wires checked and found intact","2025-03-26T08:00:00","","Completed","2025-03-25T08:00:00","No","No","No","Internal"]
[null,null,null,null,48483,"50_Wed Apr 23 2025 00:24:39 GMT+0800","2025-03-27T08:00:00","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Both the boilers blown down valve, DP transmitter, low\nlevel alarm drain valves to make free / renew and make\nthe drain line clear","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Drain valves renewed with spare and cleaned the blow down the DP transmitter and the Too Low Level float chambers of both Aux Boilers.","2025-04-11T08:00:00","","Completed","2025-04-04T08:00:00","No","No","No","Internal"]
[null,null,null,null,28286,"50_Mon Jan 06 2025 14:14:39 GMT+0800","2025-01-04T08:00:00","Critical Equipment,Defect,Observation","Ship Staff","Ship Staff Insp.","Emergency Generator is hunting for frequency and voltage during idle run condition and Auto/Man changeover knob is in damage condition. Suspecting potentiometer is malfunctioning although governor has been renewed but still problem is persists. Temporarily knob is been fabricated. ","LSA / FFA","Emgcy. Systems","Equipment Related,External Factors,Inappropriate Procedure","10.16","Very High","","","Installed newly received potentiometer and test satisfactory, the speed (rpm) and frequency were steady and setting stable according to whatever changes in demand setting on the potentiometer.","2025-05-15T08:00:00","DPEO250021","Completed","2025-04-21T08:00:00","No","No","No","Internal"]
[null,null,null,null,92874,"50_Wed Apr 23 2025 02:10:05 GMT+0800","2025-03-27T08:00:00","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Make a wooden placard for hanging the items for LOTO kit","Miscellaneous","Safety / LSA / FFA","Equipment Related","","","","","Wooden board for hanging LOTO kit items was fabricated and painted with yellow colour.","2025-04-16T08:00:00","","Completed","2025-04-18T08:00:00","No","No","No","Internal"]
[null,null,null,null,32902,"50_Wed Apr 23 2025 02:15:45 GMT+0800","2025-03-27T08:00:00","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Temporary repair on No.1 LT cooler CIP inlet line same to be permanent repaired at convenient location","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Permanent hotwork repair on No.1 LT cooler CIP inlet line was done by removing the LT outlet pipe elbow section and taken to Engine Workshop and carried out welding on the new stub piece.","2025-04-26T08:00:00","","Completed","2025-04-14T08:00:00","No","No","No","Internal"]
[null,null,null,null,71995,"50_Wed Apr 23 2025 02:19:56 GMT+0800","2025-03-27T08:00:00","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Aft area of T/G vacuum condenser very dirty same to be cleaned and painted","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","Aft area of T/G vacuum condenser was cleaned and painted, both flooring and the ship side.","2025-04-26T08:00:00","","Completed","2025-04-17T08:00:00","No","No","No","Internal"]
[null,null,null,null,32414,"50_Wed Apr 23 2025 02:24:22 GMT+0800","2025-03-27T08:00:00","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Port side and stbd side scrubber tower ventilation duct isolation valve is not free same to rectified","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Port side and stbd side scrubber tower ventilation duct operating wheel (handle) freed-up to ease-up the operation.","2025-04-26T08:00:00","","Completed","2025-04-19T08:00:00","No","No","No","Internal"]
[null,null,null,null,57266,"50_Wed Apr 23 2025 02:32:50 GMT+0800","2025-03-27T08:00:00","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","No1 and No. 2 DG turbo charger casing outlet side not properly lagged, there are high temp. areas which are exposed","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","No1 and No. 2 DG turbo charger casing outlet side missing laggings in high temp. areas was installed with newly received lagging materials in Singapore.","2025-04-06T08:00:00","","Completed","2025-04-17T08:00:00","No","No","No","Internal"]
[null,null,null,null,33284,"50_Mon Jan 13 2025 21:18:58 GMT+0800","2025-01-13T08:00:00","Defect,Observation","Ship Staff","Ship Staff Insp.","In IG system, Topping up IG blower#3 motor is showing low insulation (50 Mohm)","Cargo Mach.,Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related,External Factors,Inappropriate Procedure,Human Error","8.3","Very High","","","Motor opened up and cleaned winding with and applie CFC quick dry insulation spray, reading >500MΩ. Used same motor bearings as they were still in good condition.","2025-05-30T08:00:00","","Completed","2025-04-25T08:00:00","No","No","No","Internal","Have you carried out overhauling of motor?"]
[null,null,null,null,30711,"50_Fri May 31 2024 10:01:25 GMT+0800","2024-05-30T08:00:00","Defect","Ship Staff","Ship Staff Insp.","LOW SEA CHEST FILTER FOUND HAVING HOLES.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related,External Factors,Human Error","10.31","Very High","","","Low Sea chest strainer change with new spare received .","2025-05-15T08:00:00","DPEO250031-LOW SEA CHEST SUCTION STRAINER","Completed","2025-04-25T08:00:00","No","No","No","Internal","Spares on order."]
[null,null,null,null,16509,"50_Wed Jan 08 2025 16:59:56 GMT+0800","2025-01-04T08:00:00","Defect,Observation","Ship Staff","Ship Staff Insp.","Observed insert on IG Overboard drain line.","Miscellaneous,E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related,External Factors,Human Error","10.32","Very High","","","IG overboard sea water pipe line repaired.","2025-05-30T08:00:00","","Completed","2025-04-25T08:00:00","No","No","No","Internal"]
[null,null,null,null,89229,"50_Wed Apr 23 2025 00:33:16 GMT+0800","2025-03-27T08:00:00","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","M/E scavenge drain separator 4 alarms to try out in anchorage.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","All four alarms tried out working in order. ","2025-04-30T08:00:00","","Completed","2025-04-18T08:00:00","No","No","No","Internal"]
[null,null,null,null,10042,"50_Sat Mar 08 2025 08:42:45 GMT+0800","2025-02-27T08:00:00","Observation","Ship Staff","Ship Staff Insp.","There is a high level alarm (horn and light) fitted in bridge front (separate unit from overfill alarm), light of this unit is inoperational.","Miscellaneous","Cargo / Ballast Systems","Equipment Related","","","","","Cargo high level alarm light new spare fitted on bridge, found base damaged, same base fabricated. alarm tried out, working in good order.","2025-05-27T08:00:00","","Completed","2025-04-26T08:00:00","No","No","No","Internal"]
[null,null,null,null,43743,"50_Wed Jan 22 2025 18:39:20 GMT+0800","2025-01-21T08:00:00","Observation","Ship Staff","Ship Staff Insp.","PA system not working properly at times.","Miscellaneous","Communication","Equipment Related","","","","","Noticed mic switch not functioning, opened and reassemble switch mechanism. system  working in good order.","2025-04-30T08:00:00","","Completed","2025-04-25T08:00:00","No","No","No","Internal","What is outcome of the troubleshooting"]
[null,null,null,null,79966,"50_Sat Dec 21 2024 20:31:59 GMT+0800","2024-12-03T08:00:00","Observation","Ship Staff","Ship Staff Insp.","The Flow control valve FCV 1211 in pump room does not operate automatically","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","As of now,PCB of magnet push button is malfunctioning and valve is operated via manual hand pump. service engineer attended and mentioned that no pcb problem and fill vale has to be renewed.\n\nTransferred PCB from Filter valve BT-1211 to FCV-1211. FCV-1211 Calibrated. Valve working satisfactory.","2025-04-30T08:00:00","DPEO250114","Completed","2025-04-30T08:00:00","No","No","No","Internal","Spares on order."]
[null,null,null,null,72328,"50_Mon Jul 15 2024 23:29:51 GMT+0800","2024-07-02T08:00:00","Defect","Ship Staff","Ship Staff Insp.","No draft reading on SAAB radar system.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","SAAB radar system onboard does not calculate and display F, A & Midship drafts. The draft has to be input, manually on display. Techicians arranged for the same but the issue still persists. Office correspondence in progress.\n\nReceived new draft sensors. Draft sensor for port mid ship renewed. Still the reading of midship port is not showing. Trouble shooting in progress\n\n24.04.2025 - Draft sensor for stbd renewed.  Now all draft FWD, AFT, PORT & STBD drafts are showing. Mid ship stbd draft gauge needs calibration. Vessel will carry out calibration at load port berth.\n\nRenewal of Draft guage sensors for Port and Stbd draft guages carried out. System tested. Now all 4 drafts showing on Saab Screen","2025-05-10T08:00:00","","Completed","2025-04-26T08:00:00","No","No","Yes","Internal"]
[null,null,null,null,73450,"50_Wed Apr 23 2025 02:35:51 GMT+0800","2025-03-27T08:00:00","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Cable ducts, many places the wire passing through bulkhead doesn’t have fire class putty/cement same to be filled.","Accommodation","ISM Related","Equipment Related","","","","","Cement filler was received in Singapore. Coverred all areas on each deck that were showing even slight evidence of breach.","2025-04-26T08:00:00","","Completed","2025-04-25T08:00:00","No","No","No","Internal"]
[null,null,null,null,77920,"50_Sat Mar 15 2025 21:52:37 GMT+0800","2025-01-16T08:00:00","Defect,Observation","Ship Staff","Ship Staff Insp.","Control air dryer and filter is leaking for air.\n","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related,External Factors,Inappropriate Procedure","10.32","Very High","","","Filter dryer set of spares received in Singapore. Renewed the filter and gasket, tested and found working satisfactory.","2025-05-15T08:00:00","DPEO250080","Completed","2025-04-29T08:00:00","No","No","No","Internal"]
[null,null,null,null,68276,"50_Wed Jan 15 2025 14:19:23 GMT+0800","2025-01-14T08:00:00","Defect,Observation","Ship Staff","Ship Staff Insp.","Refrigerant Control Air Dryer is out of operation.","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related,External Factors,Human Error","10.32","Very High","","","Vessel has checked and found in/out air filters are in bad condition and Auto drain valve is malfunctioning. Dryer is giving E03 Alarm. Spares received in Singapore and installed in the unit, function tested satisfactory.","2025-05-30T08:00:00","DPEO250073","Completed","2025-04-30T08:00:00","No","No","No","Internal"]
[null,null,null,null,96672,"50_Mon Feb 24 2025 17:03:54 GMT+0800","2025-02-17T08:00:00","Defect","Ship Staff","Ship Staff Insp.","MAC #1,Compressor HP valve seat collar is damaged on cylinder block.","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related,External Factors,Inappropriate Procedure","10.32","Very High","","","Existing Cylinder block was refurbished by lapping the leaky seat. Tested compressor and working satisfactory. ","2025-05-16T08:00:00","DPEO250121","Completed","2025-04-28T08:00:00","No","No","No","Internal"]
[null,null,null,null,27348,"50_Mon Jan 13 2025 01:50:36 GMT+0800","2025-01-13T08:00:00","Observation","Ship Staff","Ship Staff Insp.","Various outfitting's on provision cranes (hook safety latch, limit switch, breather cap, connections, gauges, levers etc) require renewal.","Miscellaneous","General Appearance","Equipment Related","","","","","Limit switches was overhauled and freed-up.  Operating lever was changed with modified stick. Crane tested and working satisfactory.","2025-05-30T08:00:00","","Completed","2025-04-28T08:00:00","No","No","No","Internal","Send a separate mail for health check of crane andi n that mail mention which parts need renewal."]
[null,null,null,null,24707,"50_Thu Jan 09 2025 23:52:04 GMT+0800","2025-01-09T08:00:00","Defect,Observation","Ship Staff","Ship Staff Insp.","While Carrying out STP cleaning ,found that chlorine tablet chlorinator chamber is in damaged condition ,","Miscellaneous,Critical Equip.","MARPOL Related","Equipment Related,External Factors,Human Error","10.32","Very High","","","Fabricated chlorinator chamber using acrylic plates. Function tested and found working satisfactory. ","2025-04-30T08:00:00","DPEO250059","Completed","2025-04-23T08:00:00","No","No","No","Internal","Spares on order."]
[null,null,null,null,37710,"50_Tue Sep 03 2024 08:03:37 GMT+0800","2024-08-20T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Control air compressor not operational at engine room temperature above 33°C","E/R - Aux. Mach.,E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related,External Factors,Human Error","10.32","Very High","","","Carried out troubleshooting and found that the compressor both LO and after coolers need to be renewed.  \n- New LO after cooler received in Singpore, and installed in the Unit. Tested and found working satisfactory. ","2025-04-30T08:00:00","DPEO250095","Completed","2025-04-30T08:00:00","No","No","No","Internal","Spares on order."]
[null,null,null,null,51408,"50_Wed Jan 22 2025 02:28:52 GMT+0800","2025-01-17T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Aux Boiler LSMGO Main in-line FO Flowmeter consumption reading is erratic","E/R - Boiler,E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related,External Factors,Human Error","10.32","Very High","","","Cleaned the in-line filter of the flowmeter and tried to calibrated. Tested and found working satisfactory.","2025-05-22T08:00:00","DPEO250094","Completed","2025-04-01T08:00:00","No","No","No","Internal","Order new flowmeter."]
[null,null,null,null,92556,"50_Tue Apr 08 2025 14:50:50 GMT+0800","2025-04-08T08:00:00","Defect","Ship Staff","Ship Staff Insp.","5P & 5S WBT showing erratic sounding in SAAB system.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","10.32","Very High","","","Radar Antenna cleaned and presently all value are showing correctly and in range.","2025-05-30T08:00:00","DPEO250186 ","Completed","2025-04-22T08:00:00","No","No","No","Internal"]
[null,null,null,null,38049,"50_Mon Apr 07 2025 17:35:03 GMT+0800","2025-04-07T08:00:00","Observation","Ship Staff","Ship Staff Insp.","MF/HF Tx antenna cracked at one place. Antenna whip is supported by a clamping arrangement.","Navigation - GMDSS & Communication","Communication","Equipment Related","","","","","Fabricated new permanent support. System working satisfactory.","2025-06-19T08:00:00","DPEO250185","Completed","2025-04-07T08:00:00","No","No","No","Internal"]
[null,null,null,null,26115,"50_Sat Mar 08 2025 08:45:51 GMT+0800","2025-03-03T08:00:00","Observation","Ship Staff","Ship Staff Insp.","Nautical alarm unit showing false alarms for X band radar and Gyro off course, there are no actual on any of the equipment.","Navigation - Others","Navigation","Equipment Related","","","","","Tightened all the terminal connections and alarm reseted.","2025-05-31T08:00:00","","Completed","2025-03-20T08:00:00","No","No","No","Internal"]
[null,null,null,null,70135,"50_Sun Mar 02 2025 12:13:02 GMT+0800","2025-03-01T08:00:00","Defect,Observation","Ship Staff","Ship Staff Insp.","In ER,Out of 17 SLC column,11 column having minor defects.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related,External Factors,Inappropriate Procedure","10.32","Very High","","","Spare Power Supply Unit found from another spare part box used and installed in the unit. Fused lights and Hooter was changed. All functions satisfactory.","2025-06-01T08:00:00","DPEO250137","Completed","2025-03-03T08:00:00","No","No","No","Internal"]
[null,null,null,null,63337,"50_Sat Feb 08 2025 16:04:51 GMT+0800","2025-02-06T08:00:00","Observation","Ship Staff","Ship Staff Insp.","CCR PANEL AIR REGULATOR DIAPHRAGM LEAKING","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.11","Medium","","","Replaced with discovered spare in the B-deck. Tested and found on leak.","2025-05-30T08:00:00","DPEO250106","Completed","2025-04-22T08:00:00","No","No","No","Internal","Spares on order."]
[null,null,null,null,72689,"0_Mon Jan 13 2025 01:40:08 GMT+0800","2025-01-13T08:00:00","Observation","Ship Staff","Ship Staff Insp.","Only Cargo Pump #2 and Ballast Pump #2 vibration meter LED is malfunctioning.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","Sensor gap was adjusted in the Pumproom, and system restarted all working satisfactory.","2025-05-30T08:00:00","DPEO250133","Completed","2025-04-08T08:00:00","No","No","No","Internal","Any trouble shooting carried out? What is outcome."]
[null,null,null,null,70349,"50_Sat Jan 04 2025 20:14:53 GMT+0800","2025-01-04T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Both Aux boiler Fuel Oil Flowmeter and Running Hour meter unit is malfunctioning.","Cargo Mach.,E/R - Boiler","Eng. / Strg. Comp.","Equipment Related,External Factors,Human Error,Industry Issue","10.32","Very High","","","Service technician attended the issue in Singpore, presently showing proper values.","2025-04-30T08:00:00","DPEO250094","Completed","2025-03-27T08:00:00","No","No","No","Internal","Raise RO for same"]
[null,null,null,null,69142,"50_Mon Jan 13 2025 21:26:43 GMT+0800","2025-01-13T08:00:00","Defect,Observation","Ship Staff","Ship Staff Insp.","On deck,The main line vent valve in the IG system is seized.","Cargo Mach.,Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related,External Factors,Human Error","8.3","Very High","","","Eased-up the butterfly valve DN50 and tested working satisfactory.","2025-05-15T08:00:00","","Completed","2025-04-21T08:00:00","No","No","No","Internal"]
[null,null,null,null,19093,"50_Thu Jan 09 2025 23:17:49 GMT+0800","2025-01-06T08:00:00","Observation,Defect","Ship Staff","Ship Staff Insp.","While Carrying out LO purifier #2 4000 hours ,it was found that Lock ring for the bowl was damaged and not giving proper locking arrangment to bowl.","E/R - Purifier","","Equipment Related,External Factors,Human Error","10.32","Very High","","","Spare lock ring was been received  in Singpore, renewed and tested, now working satisfactory.","2025-05-30T08:00:00","DPEO250050","Completed","2025-03-27T08:00:00","No","No","No","Internal","Spare on order."]
[null,null,null,null,60692,"50_Sun Dec 22 2024 14:23:16 GMT+0800","2024-12-03T08:00:00","Observation","Ship Staff","Ship Staff Insp.","Chokes to be bypassed for lights on Ships.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","All the light fittings conveted from flourescent to LED as per company standard.","2025-05-10T08:00:00","","Completed","2025-04-29T08:00:00","No","No","No","Internal"]
[null,null,null,null,96110,"50_Sat Jan 04 2025 20:09:52 GMT+0800","2025-01-04T08:00:00","Critical Equipment,Observation,Defect","Ship Staff","Ship Staff Insp.","In Sewage treatment Plant, Chlorination chamber outlet valve is badly leaking from body.","Critical Equip.","MARPOL Related","Equipment Related,Human Error,External Factors","10.32","Very High","","","The valve was removed and repaired.","2025-05-15T08:00:00","DPEO250059","Completed","2025-03-19T08:00:00","No","No","No","Internal","Mention RO number."]
[null,null,null,null,16323,"50_Mon Jan 06 2025 15:43:31 GMT+0800","2025-01-04T08:00:00","Defect,Observation","Ship Staff","Ship Staff Insp.","ME Nabteso Panel and on Emergency manoeuvering panel,some of the LED's & Push button LED's is malfunctioning.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related,External Factors,Human Error","10.32","Very High","","","Changed with spare LED.","2025-05-30T08:00:00","DPEO250020","Completed","2025-04-30T08:00:00","No","No","No","Internal","Waiting for suitable quote. Send a seperate mail to take advise from nabtesco."]
[null,null,null,null,95620,"50_Sat Jan 04 2025 20:12:44 GMT+0800","2025-01-04T08:00:00","Defect,Observation","Ship Staff","Ship Staff Insp.","In BWTS unit, Aft Peak tank filter unit backflushing display monitor is erratic","Cargo Mach.","Cargo / Ballast Systems","Equipment Related,External Factors,Inappropriate Procedure","6.21","High","","","Display terminal tightened and the error was rectified.","2025-05-30T08:00:00","DPEO250060","Completed","2025-04-29T08:00:00","No","No","No","Internal","No RO number mentioned."]
[null,null,null,null,50188,"50_Wed Apr 30 2025 04:21:36 GMT+0800","2025-03-16T08:00:00","Defect","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","Seriously Steam leakage was found from the valve of steam line closed to the No. boiler at the time of inspection, which was said\nfrom the noon time before inspection","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","2.4","Medium","","","Seriously Steam leakage was found from the valve of steam line closed to the No. boiler at the time of inspection, which was said\nfrom the noon time before inspection","2025-04-15T08:00:00","","Completed","2025-03-17T08:00:00","No","No","No","External"]
[null,null,null,null,59670,"50_Wed Apr 30 2025 04:25:10 GMT+0800","2025-03-16T08:00:00","Observation","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","The round bar under port side life boat was seriously rusted which was used for ladder rigged during the course of lifeboat\nboarding.","Deck - Pipe / Fittings","","Equipment Related","5.4","High","","","Corrective Action\nAfter the operation, during the ballast passage, the round bar and outfitting near the ship’s side were de-rusted and painted. The\nround bar's condition was verified to be smooth to prevent chafing of the embarkation ladder when rigged.\nPreventative Action\nThe round bar at the starboard-side lifeboat embarkation ladder was inspected and found in good condition. Similarly, the round\nbars along the ship’s side (Pilot ladder/FWD embarkation ladder) were inspected and confirmed to be rust-free and in good order.","2025-03-30T08:00:00","","Completed","2025-03-22T08:00:00","No","No","No","External"]
[null,null,null,null,91497,"50_Wed Apr 30 2025 04:28:58 GMT+0800","2025-03-16T08:00:00","Observation","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","The spare manifold reducer, spool piece or other item of portable pipeworks were not clearly mentioned in the company\nprocedure that pressure test should be carried out to 100/% MAWP within one year period.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","6.12","Medium","","","Corrective Action\nThe replacement pump along with the required accessories were connected at the at Singapore on 27th March\n2025. Testing of all reducers carried out with the test kit.\nPreventative Action\nOnce the replacement pump is received, the reducers will be tested. The test date and pressure will be marked on them, and\nrecords will be maintained.","2025-04-12T08:00:00","","Completed","2025-04-04T08:00:00","No","No","No","External"]

{"sheet":"Calc","index":2,"n_rows":28,"n_cols":12,"rows_kept":28,"cut":false,"hidden":true,"merged":[]}
["Def_type","Def_cause","Equipments","VIQrefno","Observer_code"]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,"Dim itemSele As Long"]
[null,null,null,null,null,null,null,null,null,null,null,"   dim startRow as integer"]
[null,null,null,null,null,null,null,null,null,null,null,"   startRow=1"]
[null,null,null,null,null,null,null,null,null,null,null,"        For itemSele = 0 To ListBox1.ListCount - 1"]
[null,null,null,null,null,null,null,null,null,null,null,"        If ListBox1.Selected(itemSele) = True Then"]
[null,null,null,null,null,null,null,null,null,null,null,"        Worksheets(\"WorksheetName\").Range(\"A\" & startRow).Value = ListBox1.List(itemSele)"]
[null,null,null,null,null,null,null,null,null,null,null,"        startRow = startRow + 1"]
[null,null,null,null,null,null,null,null,null,null,null,"        End If"]
[null,null,null,null,null,null,null,null,null,null,null,"        Next"]
[null,null,null,null,null,null,null,null,null,null,null,"Dim LastRowA As String"]
[null,null,null,null,null,null,null,null,null,null,null,"        Dim itemSele As Long"]
[null,null,null,null,null,null,null,null,null,null,null,"       Dim startRow as integer"]
[null,null,null,null,null,null,null,null,null,null,null,"        LastRowA = ActiveSheet.Cells(Rows.count, \"A\").End(xlUp).row"]
[null,null,null,null,null,null,null,null,null,null,null,"        startQue = 0"]
[null,null,null,null,null,null,null,null,null,null,null,"        For itemSele = 0 To ListBox1.ListCount - 1"]
[null,null,null,null,null,null,null,null,null,null,null,"        For startRow = 1 To LastRowA"]
[null,null,null,null,null,null,null,null,null,null,null,"        If Worksheets(\"WorksheetName\").Range(\"A\" & startRow).Value = ListBox1.List(itemSele) Then"]
[null,null,null,null,null,null,null,null,null,null,null,"        ListBox1.Selected(itemSele) = True"]
[null,null,null,null,null,null,null,null,null,null,null,"        Exit For"]
[null,null,null,null,null,null,null,null,null,null,null,"        End If"]
[null,null,null,null,null,null,null,null,null,null,null,"        Next j"]
[null,null,null,null,null,null,null,null,null,null,null,"        Next"]
[null,null,null,null,null,null,null,null,null,null,null,"        End If"]

{"sheet":"Areaofobs","index":3,"n_rows":17,"n_cols":2,"rows_kept":17,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Cargo / Ballast Systems",11]
["Cert. & Docu.",2]
["Communication",6]
["Crew Management",3]
["Emgcy. Systems",13]
["Eng. / Strg. Comp.",14]
["General Appearance",15]
["Ice Opns.",17]
["ISM Related",7]
["ISPS Related",10]
["MARPOL Related",9]
["MLC Related",4]
["Mooring",12]
["Navigation",5]
["Safety / LSA / FFA",8]
["Structural Condn. / WT integrity ",16]

{"sheet":"Vessel_type","index":4,"n_rows":1,"n_cols":2,"rows_kept":1,"cut":false,"hidden":true,"merged":[]}
["Vessel_type","ID"]

{"sheet":"Deficiency_type","index":5,"n_rows":8,"n_cols":3,"rows_kept":8,"cut":false,"hidden":true,"merged":[]}
["TITLE","Type of deficiency_description","ID"]
["Breakdown",null,6]
["Critical Equipment",null,4]
["Defect",null,1]
["Guarantee Claim",null,8]
["Non Conformity",null,2]
["Observation",null,3]
["Other",null,7]

{"sheet":"VIQrefno","index":6,"n_rows":427,"n_cols":3,"rows_kept":427,"cut":false,"hidden":true,"merged":[]}
["VIQ_ref_no","Risk Value of observation","ID"]
["1.1","Low",8243]
["1.10","Low",8252]
["1.11","Low",8253]
["1.12","Low",8254]
["1.13","Low",8255]
["1.14","Low",8256]
["1.15","Low",8257]
["1.16","Low",8259]
["1.17","Low",8260]
["1.18","Low",8261]
["1.19","Low",8262]
["1.2","Low",8244]
["1.20","Low",8263]
["1.21","Low",8265]
["1.22","Low",8266]
["1.23","Low",8267]
["1.24","Low",8268]
["1.25","Low",8269]
["1.26","Low",8270]
["1.3","Low",8245]
["1.4","Low",8246]
["1.5","Low",8247]
["1.6","Low",8248]
["1.7","Low",8249]
["1.8","Low",8250]
["1.9","Low",8251]
["1.99","High",11258]
["10.1","Medium",8461]
["10.10","High",8470]
["10.11","Medium",8471]
["10.12","Very High",8472]
["10.13","Very High",8473]
["10.14","Medium",8474]
["10.15","Low",8475]
["10.16","Very High",8476]
["10.17","Very High",8477]
["10.18","High",8478]
["10.19","Very High",8479]
["10.2","Low",8462]
["10.20","High",8480]
["10.21","Medium",8481]
["10.22","Low",8482]
["10.23","Medium",8483]
["10.24","Low",8484]
["10.25","Very High",8485]
["10.26","High",8486]
["10.27","Medium",8487]
["10.28","Low",8488]
["10.29","Medium",8489]
["10.3","Medium",8463]
["10.30","High",8490]
["10.31","Very High",8491]
["10.32","Very High",8492]
["10.33","High",8493]
["10.34","High",8494]
["10.35","Very High",8495]
["10.36","Very High",8496]
["10.37","Medium",8497]
["10.38","Medium",8498]
["10.39","High",8499]
["10.4","High",8464]
["10.40","Medium",8500]
["10.41","Medium",8501]
["10.42","Medium",8502]
["10.43","Medium",8503]
["10.44","Medium",8504]
["10.45","Very High",8505]
["10.46","High",8506]
["10.47","Medium",8507]
["10.48","High",8508]
["10.49","Medium",8509]
["10.5","Low",8465]
["10.50","High",8510]
["10.51","Low",8511]
["10.52","Medium",8512]
["10.53","Medium",8513]
["10.54","High",8514]
["10.55","Low",8515]
["10.6","Very High",8466]
["10.7","Medium",8467]
["10.8","Medium",8468]
["10.9","Medium",8469]
["10.99","High",8516]
["11.1","High",8420]
["11.10","Medium",8429]
["11.11","Very High",8430]
["11.12","Low",8431]
["11.13","Low",8432]
["11.14","Medium",8433]
["11.15","Low",8434]
["11.16","Low",8435]
["11.17","Low",8436]
["11.2","Medium",8421]
["11.3","Medium",8422]
["11.4","Very High",8423]
["11.5","Medium",8424]
["11.6","Medium",8425]
["11.7","High",8426]
["11.8","Low",8427]
["11.9","Low",8428]
["11.99","High",8437]
["12.1","High",8438]
["12.10","High",8448]
["12.11","High",8449]
["12.12","High",8450]
["12.13","High",8451]
["12.14","High",8452]
["12.15","High",8453]
["12.16","High",8454]
["12.17","High",8455]
["12.18","High",8456]
["12.19","High",8457]
["12.2","High",8439]
["12.20","High",8458]
["12.21","High",8459]
["12.3","High",8441]
["12.4","High",8442]
["12.5","High",8443]
["12.6","High",8444]
["12.7","High",8445]
["12.8","High",8446]
["12.9","High",8447]
["12.99","High",8460]
["2.1","Very High",8296]
["2.1.9","Very High",11259]
["2.10","Medium",8304]
["2.11","Medium",8305]
["2.12","Low",8306]
["2.13","Low",8307]
["2.14","Low",8308]
["2.15","Low",8309]
["2.16","Medium",8310]
["2.2","Medium",8297]
["2.3","High",8295]
["2.4","Medium",8298]
["2.5","Medium",8299]
["2.6","Low",8300]
["2.7","High",8301]
["2.8","High",8302]
["2.9","Medium",8303]
["2.99","High",8311]
["3.1","High",8312]
["3.2","Very High",8313]
["3.3","High",8314]
["3.4","Low",8294]
["3.5","Medium",8315]
["3.6","High",8316]
["3.7","Very High",8317]
["3.8","Very High",8318]
["3.99","High",8319]
["4.1","High",8320]
["4.10","High",8329]
["4.11","Medium",8330]
["4.12","Very High",8331]
["4.13","Very High",8332]
["4.14","Very High",8333]
["4.15","Very High",8334]
["4.16","Very High",8335]
["4.17","Very High",8336]
["4.18","Very High",8337]
["4.19","Low",8338]
["4.2","Medium",8321]
["4.20","Very High",8339]
["4.21","High",8340]
["4.22","Low",8341]
["4.23","High",8342]
["4.24","High",8343]
["4.25","Low",8344]
["4.26","Low",8345]
["4.27","High",8346]
["4.3","Medium",8322]
["4.4","High",8323]
["4.5","Very High",8324]
["4.6","Medium",8325]
["4.7","High",8326]
["4.8","Medium",8327]
["4.9","Medium",8328]
["4.99","High",8347]
["5.1","Very High",8517]
["5.10","High",8526]
["5.11","Low",8527]
["5.12","Medium",8528]
["5.13","High",8529]
["5.14","Very High",8530]
["5.15","Medium",8531]
["5.16","Very High",8532]
["5.17","Very High",8533]
["5.18","High",8534]
["5.19","Medium",8535]
["5.2","Very High",8518]
["5.20","Medium",8536]
["5.21","Medium",8537]
["5.22","High",8539]
["5.23","Very High",8540]
["5.24","Very High",8541]
["5.25","Medium",8542]
["5.26","Medium",8543]
["5.27","Medium",8544]
["5.28","Very High",8545]
["5.29","High",8546]
["5.3","Low",8519]
["5.30","High",8547]
["5.31","High",8548]
["5.32","High",8549]
["5.33","High",8550]
["5.34","Low",8551]
["5.35","Medium",8552]
["5.36","Low",8553]
["5.37","Low",8554]
["5.38","High",8555]
["5.39","Very High",8556]
["5.4","High",8520]
["5.40","Very High",8557]
["5.41","Very High",8558]
["5.42","Medium",8559]
["5.43","High",8560]
["5.44","High",8561]
["5.45","Medium",8564]
["5.46","Medium",8565]
["5.47","Medium",8566]
["5.48","Medium",8567]
["5.5","Low",8521]
["5.6","Low",8522]
["5.7","Medium",8523]
["5.8","Medium",8524]
["5.9","Very High",8525]
["5.99","High",8568]
["6.1","Medium",8348]
["6.10","Low",8357]
["6.11","High",8358]
["6.12","Medium",8359]
["6.13","Low",8360]
["6.14","High",8361]
["6.15","High",8362]
["6.16","Very High",8363]
["6.17","Very High",8364]
["6.18","Medium",8365]
["6.19","Low",8366]
["6.2","High",8349]
["6.20","Medium",8367]
["6.21","High",8368]
["6.22","Medium",8369]
["6.3","Low",8350]
["6.4","High",8351]
["6.5","Medium",8352]
["6.6","Medium",8353]
["6.7","High",8354]
["6.8","High",8355]
["6.9","Low",8356]
["6.99","High",8370]
["7.1","High",8371]
["7.10","High",8380]
["7.11","High",8381]
["7.12","High",8382]
["7.13","Medium",8383]
["7.14","Medium",8384]
["7.15","High",8385]
["7.16","High",8386]
["7.17","High",8387]
["7.2","High",8372]
["7.3","Low",8373]
["7.4","Low",8374]
["7.5","Low",8375]
["7.6","Medium",8376]
["7.7","Low",8377]
["7.8","High",8378]
["7.9","High",8379]
["7.99","High",8388]
["8.1","Very High",8569]
["8.10","Very High",8578]
["8.100","Low",11227]
["8.101","Medium",11228]
["8.102","Low",11229]
["8.103","Low",11230]
["8.104","Low",11231]
["8.105","Medium",11232]
["8.106","Medium",11233]
["8.107","Low",11234]
["8.108","High",11235]
["8.109","Very High",11236]
["8.11","Medium",8579]
["8.110","High",11237]
["8.111","Medium",11238]
["8.112","High",11239]
["8.113","Medium",11240]
["8.114","Low",11241]
["8.115","High",11242]
["8.116","Medium",11243]
["8.117","Medium",11244]
["8.118","Medium",11245]
["8.119","High",11246]
["8.12","Medium",8580]
["8.120","High",11247]
["8.121","Medium",11248]
["8.122","High",11249]
["8.123","High",11250]
["8.124","Low",11251]
["8.125","High",11252]
["8.126","Medium",11253]
["8.127","Medium",11254]
["8.13","Medium",8581]
["8.14","Very High",8582]
["8.15","High",8583]
["8.16","Very High",8584]
["8.17","Low",8585]
["8.18","High",8586]
["8.19","High",8587]
["8.199","High",11255]
["8.2","Medium",8570]
["8.20","Medium",8588]
["8.21","High",8589]
["8.22","Very High",8590]
["8.23","Medium",8591]
["8.24","Medium",8592]
["8.25","Very High",8593]
["8.26","High",8594]
["8.27","Medium",8595]
["8.28","Medium",8596]
["8.29","High",8598]
["8.3","Very High",8571]
["8.30","High",8599]
["8.31","High",8600]
["8.32","Low",8601]
["8.33","Medium",8602]
["8.34","High",8603]
["8.35","Medium",8604]
["8.36","Medium",8605]
["8.37","High",8607]
["8.38","Medium",8608]
["8.39","Medium",8609]
["8.4","Medium",8572]
["8.40","High",8610]
["8.41","Medium",8611]
["8.42","Medium",8612]
["8.43","Very High",8613]
["8.44","High",8615]
["8.45","High",8616]
["8.46","Very High",8617]
["8.47","Very High",8618]
["8.48","Medium",8619]
["8.49","High",8620]
["8.5","Very High",8573]
["8.50","Medium",8621]
["8.51","Low",8622]
["8.52","Low",8623]
["8.53","Low",8624]
["8.54","High",8625]
["8.55","Low",11182]
["8.56","Medium",11183]
["8.57","Medium",11184]
["8.58","High",11185]
["8.59","High",11186]
["8.6","Medium",8574]
["8.60","High",11187]
["8.61","Medium",11188]
["8.62","Very High",11189]
["8.63","High",11190]
["8.64","Medium",11191]
["8.65","Low",11192]
["8.66","High",11193]
["8.67","High",11194]
["8.68","High",11195]
["8.69","Medium",11196]
["8.7","High",8575]
["8.70","Medium",11197]
["8.71","Very High",11198]
["8.72","Medium",11199]
["8.73","Medium",11200]
["8.74","High",11201]
["8.75","Medium",11202]
["8.76","Medium",11203]
["8.77","Medium",11204]
["8.78","Medium",11205]
["8.79","Medium",11206]
["8.8","Medium",8576]
["8.80","Medium",11207]
["8.81","Low",11208]
["8.82","Medium",11209]
["8.83","Low",11210]
["8.84","Low",11211]
["8.85","Medium",11212]
["8.86","Medium",11213]
["8.87","Medium",11214]
["8.88","Low",11215]
["8.89","High",11216]
["8.9","High",8577]
["8.90","High",11217]
["8.91","High",11218]
["8.92","Medium",11219]
["8.93","Low",11220]
["8.94","Low",11221]
["8.95","Medium",11222]
["8.96","Medium",11223]
["8.97","Low",11224]
["8.98","High",11225]
["8.99","Medium",11226]
["9.1","Low",8390]
["9.10","Medium",8399]
["9.11","Medium",8400]
["9.12","Medium",8401]
["9.13","Low",8402]
["9.14","Medium",8403]
["9.15","Medium",8404]
["9.16","High",8405]
["9.17","High",8406]
["9.18","Low",8407]
["9.19","Low",8408]
["9.2","Very High",8391]
["9.20","Medium",8409]
["9.21","Medium",8410]
["9.22","Low",8411]
["9.23","Low",8412]
["9.24","Medium",8413]
["9.25","Low",8414]
["9.26","Low",8415]
["9.27","Low",8416]
["9.28","Medium",8417]
["9.29","Low",8418]
["9.3","Very High",8392]
["9.4","High",8393]
["9.5","High",8394]
["9.6","Low",8395]
["9.7","Medium",8396]
["9.8","Medium",8397]
["9.9","Medium",8398]
["9.99","High",8419]

{"sheet":"Equipment_list","index":7,"n_rows":28,"n_cols":3,"rows_kept":28,"cut":false,"hidden":true,"merged":[]}
["TITLE","Equipment_list_description","ID"]
["Accommodation",null,12]
["Cargo Mach.",null,13]
["Critical Equip.",null,16]
["Deck - Machinery",null,18]
["Deck - Mooring Machinery",null,15]
["Deck - Pipe / Fittings",null,20]
["Documentation",null,21]
["E/R - Air Comp.",null,8]
["E/R - Aux. Engine",null,4]
["E/R - Aux. Mach.",null,7]
["E/R - Boiler",null,5]
["E/R - Main Engine",null,3]
["E/R - Pipes/ valves & fittings",null,9]
["E/R - Pumps",null,32]
["E/R - Purifier",null,6]
["Elect. Mach. & Equip.",null,10]
["Hull & Tanks",null,19]
["Inert Gas",null,14]
["LSA / FFA",null,17]
["Miscellaneous",null,22]
["Navigation - DGPS / EPFS / AIS",null,28]
["Navigation - ECDIS",null,25]
["Navigation - Echo Sounder / Speed Log",null,26]
["Navigation - GMDSS & Communication",null,23]
["Navigation - Others",null,11]
["Navigation - RADAR",null,24]
["Navigation - VDR / BNWAS",null,30]

{"sheet":"PSC_MOU","index":8,"n_rows":11,"n_cols":3,"rows_kept":11,"cut":false,"hidden":true,"merged":[]}
["TITLE","PSC_MOU_description","ID"]
["Asia and the Pacific",null,2]
["Caribbean",null,4]
["Europe and the North Atlantic",null,1]
["Latin America",null,3]
["The Black Sea region",null,6]
["The Indian Ocean",null,8]
["The Mediterranean",null,7]
["The Riyadh MoU",null,9]
["USCG",null,10]
["West and Central Africa",null,5]

{"sheet":"Inspection_type","index":9,"n_rows":14,"n_cols":2,"rows_kept":14,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Bunkering Audit",14]
["Cargo Audit",17]
["Engineering Audit",16]
["ISM Audit",2]
["ISPS Audit",3]
["IT Audit",10]
["MLC Audit",1]
["Mooring Audit",9]
["Nav Audit / Verification",8]
["Onboard Training",18]
["PSC Inspection",4]
["Ship Staff Insp.",15]
["Suptd. Insp.",13]

{"sheet":"Deficiency_Cause","index":10,"n_rows":8,"n_cols":3,"rows_kept":8,"cut":false,"hidden":true,"merged":[]}
["TITLE","Deficiency_Cause_description","ID"]
["Behaviour Based",null,1]
["Equipment Related",null,4]
["External Factors",null,5]
["Human Error",null,7]
["Inappropriate Procedure",null,8]
["Industry Issue",null,6]
["Knowledge Based",null,3]

{"sheet":"Observer_code","index":11,"n_rows":3,"n_cols":3,"rows_kept":3,"cut":false,"hidden":true,"merged":[]}
["TITLE","Observer_code_description","ID"]
["Owner / Marine / Tech. Suptd.",null,3]
["Ship Staff",null,2]

{"sheet":"Status_code","index":12,"n_rows":6,"n_cols":3,"rows_kept":6,"cut":false,"hidden":true,"merged":[]}
["TITLE","Status_code_description","ID"]
["Completed",null,6]
["Deferred to D D",null,5]
["In progress",null,3]
["Not Started",null,2]
["Waiting spare",null,4]

{"sheet":"PSC_ref_no","index":13,"n_rows":19,"n_cols":2,"rows_kept":19,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Alarms",9]
["Cargo operations including equipment",7]
["Certificates & Documentation",2]
["Dangerous Goods",13]
["Emergency Systems",5]
["Fire safety",8]
["ISM",16]
["ISPS",17]
["Life saving appliances",12]
["MLC, 2006",18]
["Other",19]
["Pollution Prevention",15]
["Propulsion and auxiliary machinery",14]
["Radio communication",6]
["Safety of Navigation",11]
["Structural condition",3]
["Water/Weathertight condition",4]
["Working and Living Conditions",10]

{"sheet":"Risk_value_of_obs","index":14,"n_rows":1,"n_cols":2,"rows_kept":1,"cut":false,"hidden":true,"merged":[]}
["Risk Value of observation","ID"]

{"sheet":"Year","index":15,"n_rows":18,"n_cols":1,"rows_kept":18,"cut":false,"hidden":true,"merged":[]}
["Year"]
[2014]
[2015]
[2016]
[2017]
[2018]
[2019]
[2020]
[2021]
[2022]
[2023]
[2024]
[2025]
[2026]
[2027]
[2028]
[2029]
[2030]

{"sheet":"Month","index":16,"n_rows":13,"n_cols":1,"rows_kept":13,"cut":false,"hidden":true,"merged":[]}
["Month"]
["Jan"]
["Feb"]
["Mar"]
["Apr"]
["May"]
["Jun"]
["Jul"]
["Aug"]
["Sep"]
["Oct"]
["Nov"]
["Dec"]

{"sheet":"Date_","index":17,"n_rows":32,"n_cols":1,"rows_kept":32,"cut":false,"hidden":true,"merged":[]}
["Date"]
["01"]
["02"]
["03"]
["04"]
["05"]
["06"]
["07"]
["08"]
["09"]
[10]
[11]
[12]
[13]
[14]
[15]
[16]
[17]
[18]
[19]
[20]
[21]
[22]
[23]
[24]
[25]
[26]
[27]
[28]
[29]
[30]
[31]

{"sheet":"Sheet1","index":18,"n_rows":24,"n_cols":6,"rows_kept":24,"cut":false,"hidden":true,"merged":[]}
[]
[null,"ID","E",null,"Date Recorded",1]
[null,"UNIQUE ID","F",null,"Type of Deficiency",2]
[1,"Date Recorded","G",null,"Observer code",3]
["ignore","Vessel Type","H",null,"Type of Inspection",4]
[null,"Internal / External","I",null,"Description of Deficiency",5]
[null,"Drydock","J",null,"Equipment Categories",6]
[null,"Information Sharing","K",null,"Area of Observation",7]
[null,"Critical_item","L",null,"Deficiency Cause",8]
[null,"Deficiency Type","M",null,"VIQ Ref Number",9]
[null,"Deficiency Cause","N",null,"Risk Value of Obs",10]
[null,"Inspection Type","O",null,"PSC Ref Number",11]
[null,"Equipments","P",null,"PSC MOU ID",12]
[null,"VIQ Reference Number","Q",null,"Action Taken or Required",13]
[null,"Risk Value of the observation","R",null,"Target Date",14]
[null,"PSC Reference Number","S",null,"PO Ref No.",15]
[null,"PSC MOU","T",null,"Status Code",16]
[null,"Observer Code","U",null,"Date Completed",17]
[null,"Target Date","V",null,"Drydock",18]
[null,"Status Code","W",null,"Info Sharing",19]
[null,"Description of Deficiency","X",null,"Critical Item Flag",20]
[null,"Action taken / required","Y",null,"Audit Type",21]
[null,"PO ref no","Z"]
[null,"Date completed","AA"]

{"sheet":"Ship_information","index":19,"n_rows":2,"n_cols":4,"rows_kept":2,"cut":false,"hidden":true,"merged":[]}
["Ship_ID","Ship_Name","FILE_NAME","Export_Date"]
["50","DHT PEONY (17-02-2025)","50_1740377401478.xlsm","2025-04-30 04:04:50"]

{"sheet":"External_Deficiency_type","index":20,"n_rows":5,"n_cols":3,"rows_kept":5,"cut":false,"hidden":true,"merged":[]}
["TITLE","Type of deficiency_description","ID"]
["Condn of Class / Memo",null,5]
["Defect",null,1]
["Non Conformity",null,2]
["Observation",null,3]

{"sheet":"External_Inspection_type","index":21,"n_rows":11,"n_cols":2,"rows_kept":11,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Cargo Audit",17]
["Flag State Insp.",5]
["ISM Audit",2]
["ISPS Audit",3]
["MLC Audit",1]
["Nav Audit / Verification",8]
["OM Insp. (Eg. SIRE / CDI etc.)",6]
["Others (Eg. Insurance etc.)",12]
["PSC Inspection",4]
["Terminal Insp.",11]

{"sheet":"External_Observer_code","index":22,"n_rows":7,"n_cols":3,"rows_kept":7,"cut":false,"hidden":true,"merged":[]}
["TITLE","Observer_code_description","ID"]
["Class Surveyor",null,4]
["FSC Inspector",null,5]
["Others (Eg. Insurance etc.)",null,9]
["PSC Insp.",null,6]
["SIRE / CDI Insp.",null,8]
["Terminal Insp.",null,7]

{"sheet":"Sheet Version","index":23,"n_rows":2,"n_cols":2,"rows_kept":2,"cut":false,"hidden":true,"merged":[]}
["Version","Title"]
["2.0","Version 2.0"]