{"text_format":"1","workbook":"xlsx","n_sheets":24,"sheets":["Mainsheet","Completed","Calc","Areaofobs","Vessel_type","Deficiency_type","VIQrefno","Equipment_list","PSC_MOU","Inspection_type","Deficiency_Cause","Observer_code","Status_code","PSC_ref_no","Risk_value_of_obs","Year","Month","Date_","Sheet1","Ship_information","External_Deficiency_type","External_Inspection_type","External_Observer_code","Sheet Version"],"not_rendered":{"charts":0,"images":1,"macros":1,"external_links":0,"defined_names":12,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Mainsheet","index":0,"n_rows":41,"n_cols":28,"rows_kept":41,"cut":false,"hidden":false,"merged":[[10,8,10,9],[10,12,10,13],[12,6,12,27],[8,6,8,27]]}
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,"Defect - Damage Monitoring Sheet"]
[]
[null,null,null,null,null,null,null,"Date of Report","01-Jul-2025",null,null,"Ship Name","DHT JAGUAR (03-05-2025)"]
[]
[null,null,null,null,null,null,"VERSION : 2.0"]
[]
[]
[]
[null,null,null,"ID","SHIPSIDE UNIQUEID","UNIQUE ID","Date Recorded","Type of Deficiency","Observer code","Type of Inspection","Description of Deficiency","Equipment Categories","Area of Observation","Deficiency Cause","VIQ Ref Number","Risk Value of Obs","PSC Ref Number","PSC MOU ID","Action Taken or Required","Target Date","PO Ref No.","Status Code","Date Completed","Drydock","Info Sharing","Critical Item","Audit Type","Superintendent Remarks"]
[null,null,null,null,35465,"30_Sat Jan 25 2025 19:26:30 GMT+0800","2025-02-21T08:00:00","Breakdown","Ship Staff","Ship Staff Insp.","Bridge wiper No.4 wiper module became faulty, Supply to motor and parking sensor is missing. Module need to be renewed.","Elect. Mach. & Equip.","Navigation","Equipment Related","12.10","High","","","Spare received in Singapore on 2nd May 2025. Vessel renewed the faulty module but same got burnt. Electrical technical support team has been notified. Investigation in progress. New RO raised DJAG250184 for wiper module.","2025-07-30T08:00:00","DJAG250184","Waiting spare",null,"No","No","No","Internal","RO  DJAG250052  is ordered. Same will be supplied to the vessel once vessel calls Singapore in May."]
[null,null,null,null,57598,"30_Wed Mar 19 2025 16:21:55 GMT+0800","2025-02-26T08:00:00","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Safety walkway hand rail forward of manifold (about 4 mtrs) found corroded, same to be de-rusted and painted.","Deck - Pipe / Fittings","General Appearance","Equipment Related","","","","","Safety walkway hand rail forward of manifold (about 4 mtrs) found corroded, same to be de-rusted and painted.","2025-06-15T08:00:00","","In progress",null,"No","No","No","Internal","Noted on Condition of Safety walkway hand rail.\nDo update the same."]
[null,null,null,null,83462,"30_Wed Mar 19 2025 15:50:38 GMT+0800","2025-02-26T08:00:00","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Anchor marking buoy not available. Same to be requisitioned.","Miscellaneous","Navigation","Equipment Related","9.21","Medium","","","Requisition raised for Anchor marking buoy DJAG250085.","2025-06-30T08:00:00","DJAG250085","In progress",null,"No","No","No","Internal","Please check on RO Number DJAG250085. The same is NOT visible in our system,"]
[null,null,null,null,22723,"30_Wed Mar 19 2025 16:29:52 GMT+0800","2025-02-26T08:00:00","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Pump room light shades / cover in spare shades not available. Vessel to order 6 pcs","Miscellaneous","Cargo / Ballast Systems","Equipment Related","","","","","RO -  DJAG250126 raised for Pump room light shades ","2025-07-30T08:00:00","DJAG250126","Waiting spare",null,"No","No","No","Internal","Please advise RO number for Pump room light shades for follow up."]
[null,null,null,null,66671,"30_Sun Mar 16 2025 23:45:04 GMT+0800","2025-02-28T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Main engine exhaust gas bypass valve found to be malfunctioning. Upon investigation observed SIPART I/P controller not working.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Vessel has raised RO DJAG240232. Awaiting for spares. Once the RO is supplied, same can be renewed by ship staff.","2025-07-30T08:00:00","DJAG240232","Not Started",null,"No","No","No","Internal","Noted on RO DJAG240232.\nPlease send follow up email to Auto Electric dept.\nInclude the defect in Refmen"]
[null,null,null,null,75823,"30_Mon Mar 10 2025 18:53:51 GMT+0800","2025-03-10T08:00:00","Breakdown","Ship Staff","Ship Staff Insp.","Common fan for smoke and officer room exhaust was found defective due rusted bearings and damaged winding insulation","Accommodation","","Equipment Related","","","","","RO has been raised. Awaiting spares.","2025-07-30T08:00:00","DJAG250082","Waiting spare",null,"No","No","No","Internal","RO DJAG250082 is noted.\nwe have received two quotes. Procure will check and send to vessel for confirm suitability"]
[null,null,null,null,45769,"30_Sun Mar 16 2025 20:39:34 GMT+0800","2025-03-30T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Main engine jacket water controller positioner is not responding to the input signal.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","ME JCW controller has been overhauled by HKT Tech in DD,but after few days controller is not responding to the signal.need to renew coil.As of now vessel has plan to swap with FWG controller during ME is in stopped condition.","2025-07-30T08:00:00","DJAG250238","Waiting spare",null,"No","No","No","Internal","One quote has been received and suitability check is in progress."]
[null,null,null,null,87107,"30_Wed May 14 2025 09:05:44 GMT+0800","2025-05-06T08:00:00","Observation","Ship Staff","Ship Staff Insp.","Fresh water tank (Port side) low level alarm switch is not operating. ","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","Requisition DJAG250181 raised. Awaiting spares.","2025-07-30T08:00:00","DJAG250181","Waiting spare",null,"No","No","No","Internal"]
[null,null,null,null,82323,"30_Mon Jun 23 2025 09:04:16 GMT+0800","2024-11-01T08:00:00","Critical Equipment,Defect","Ship Staff","Ship Staff Insp.","EGCS CEMS Peristaltic Pump (SCC condensate drain), was not draining the water, hence the water getting carried to the gas analyser unit.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","Requires regular observation and draining the water from the system.\nAwaiting for spare","2025-09-19T08:00:00","DJAG250104","Waiting spare",null,"No","No","No","Internal"]
[null,null,null,null,97472,"30_Mon Jun 23 2025 14:18:59 GMT+0800","2025-06-22T08:00:00","Defect,Observation","Ship Staff","Ship Staff Insp.","Main Engine Auto Back Wash SFF LO filter hydraulic actuator seal leaking for oil.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related,External Factors,Inappropriate Procedure","10.32","Very High","","","Hydraulic actuator unit to be overhauled.","2025-09-22T08:00:00","DJAG250233","Waiting spare",null,"No","No","No","Internal"]
[null,null,null,null,19313,"30_Thu Jun 26 2025 09:45:04 GMT+0800","2025-06-15T08:00:00","Defect","Ship Staff","Ship Staff Insp.","No.1 ECR Unit Cooler High/Low pressure controller is malfunctioning for compressor.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","As of now gas is charged in the system and system is normal.but pressure switch will not activate in case high pressure.","2025-09-15T08:00:00","DJAG250244","Waiting spare",null,"No","No","No","Internal"]
[null,null,null,null,78247,"30_Thu Jun 26 2025 10:23:32 GMT+0800","2025-05-20T08:00:00","Defect","Ship Staff","Ship Staff Insp.","COPT Vacuum condenser water level controller malfunctioning, as per shore technician in dry-dock, level controller need to be replaced.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","Control valve positioner calibrated, found satisfactory. Needed to replace level controller, requisition raised ","2025-08-20T08:00:00","DJAG250242","Waiting spare",null,"No","No","No","Internal"]
[null,null,null,null,31733,"30_Thu Jun 26 2025 21:43:52 GMT+0800","2025-05-01T08:00:00","Observation","Ship Staff","Ship Staff Insp.","High Sea chest MGPS anodes renewal.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Both anodes has been consumed by more than 80% and MGPS unit is giving alarm for low volt.\nAnodes to be renewed.","2025-07-31T08:00:00","DJAG250081","Waiting spare",null,"No","No","No","Internal"]
[null,null,null,null,75418,"30_Thu Jun 26 2025 23:16:11 GMT+0800","2025-04-01T08:00:00","Breakdown","Ship Staff","Ship Staff Insp.","ER Vacuum Toilet discharge valve is malfunctioning.","Accommodation","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Discharge valve to be renewed.","2025-07-31T08:00:00","DJAG250080","Waiting spare",null,"No","No","No","Internal"]
[null,null,null,null,56118,"30_Thu Jun 26 2025 23:18:37 GMT+0800","2025-04-30T08:00:00","Breakdown","Ship Staff","Ship Staff Insp.","In Sewage treatment Plant,EOCR are not operational, circuit modified and running on other type OCR","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Awaiting for spare","2025-07-31T08:00:00","DJAG250131","Waiting spare",null,"No","No","No","Internal"]
[null,null,null,null,89853,"30_Thu Jun 26 2025 23:23:32 GMT+0800","2025-05-31T08:00:00","Defect","Ship Staff","Ship Staff Insp.","ME LO Auto SFF bypass paper filter getting chocked frequently, Need a renewal","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","SFF bypass paper filter to be renewed.As of now vessel has 3 new spares and will renew at sea.","2025-08-31T08:00:00","DJAG250150","Waiting spare",null,"No","No","No","Internal"]
[null,null,null,null,65589,"30_Thu Jun 26 2025 23:25:14 GMT+0800","2025-05-31T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Generator lub oil purifier running on high vibration.","E/R - Purifier","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","clean/overhaul or will renew the vertical shaft bearing if reqd.","2025-08-31T08:00:00","DJAG250191","Waiting spare",null,"No","No","No","Internal"]
[null,null,null,null,42862,"30_Mon Jun 30 2025 13:40:03 GMT+0800","2025-06-29T08:00:00","Critical Equipment,Defect","Ship Staff","Ship Staff Insp.","MAIN ENGINE MINIMESS PRESSURE TEST GAUGE IS MALFUNCTIONING.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related,Human Error,Inappropriate Procedure","10.32","Very High","","","NEED A NEW PRESSURE GAUGE UNIT","2025-09-29T08:00:00","DJAG250245","Waiting spare",null,"No","No","No","Internal"]
[null,null,null,null,50573,"30_Tue Jul 01 2025 09:04:41 GMT+0800","2025-06-20T08:00:00","Critical Equipment,Defect,Observation","Ship Staff","Ship Staff Insp.","Main sea water pump and vacuum condenser sea water pump mech seal leaking.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related,Human Error,Inappropriate Procedure","10.32","Very High","","","Both pump motor has been overhauled by shore technician in DD,after installation due to motor coupling misalignment pump is started leaking through mech seal.as of now vessel need a OEM spares to overhaul the pump. ","2025-07-30T08:00:00","DJAG250187","Waiting spare",null,"No","No","No","Internal"]
[null,null,null,null,57452,"30_Tue Jul 01 2025 09:11:06 GMT+0800","2025-06-19T08:00:00","Defect,Observation","Ship Staff","Ship Staff Insp.","Main Engine EICU A MPC PCB relay unit is malfunctioning.","Critical Equip.,E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related,Inappropriate Procedure","10.32","Very High","","","After attending the SE in DD, during departure alarm is triggered on PCB relay.after discussion with technician the EICU A PCB to be replaced with spare one.","2025-09-30T08:00:00","DJAG250225","Waiting spare",null,"No","No","No","Internal"]
[null,null,null,null,38052,"30_Tue Jul 01 2025 09:13:41 GMT+0800","2025-05-20T08:00:00","Defect,Observation","Ship Staff","Ship Staff Insp.","COPT #2 & WBPT Auto Grease cup unit is in broken condition.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related,External Factors,Inappropriate Procedure","8.22","Very High","","","Both auto grease cup to be renewed.","2025-07-30T08:00:00","DJAG250202","Waiting spare",null,"No","No","No","Internal"]
[null,null,null,null,16547,"30_Tue Jul 01 2025 09:21:38 GMT+0800","2025-06-20T08:00:00","Observation,Critical Equipment","Ship Staff","Ship Staff Insp.","While running AE # 2 in parallel with other AE,after few hours running time suddenly AE #2 is tripping on preferential trip followed by high bus bar voltage. ","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related,External Factors,Human Error","10.32","Very High","","","In DD,technician haa cleaned and checked the all ACB's and in Singapore Hyundai technician has attended the vessel for parameter check. but again the issue is not resolved.vessel has checked fuel rack,governor response,duplex in line filter,FO pressure for AE #2 and found in good order.as we plan for to replace ACB with spare one.","2025-07-30T08:00:00","","In progress",null,"No","No","No","Internal"]
[null,null,null,null,77778,"30_Tue Jul 01 2025 09:33:22 GMT+0800","2025-03-03T08:00:00","Defect","Ship Staff","Ship Staff Insp.","High Sea chest MGPS anodes consumed more than 80%.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related,External Factors,Inappropriate Procedure","10.32","Very High","","","Need to be renewed complete set.","2025-07-30T08:00:00","DJAG250081","Waiting spare",null,"No","No","No","Internal"]
[null,null,null,null,97042,"30_Tue Jul 01 2025 09:36:07 GMT+0800","2025-06-20T08:00:00","Critical Equipment,Defect","Ship Staff","Ship Staff Insp.","Portable Water test chemical expired.","Miscellaneous","MLC Related","Equipment Related","10.32","Very High","","","Test Chemicals to be received.","2025-09-20T08:00:00","DJAG250071","Waiting spare",null,"No","No","No","Internal"]

{"sheet":"Completed","index":1,"n_rows":596,"n_cols":28,"rows_kept":596,"cut":false,"hidden":false,"merged":[[10,8,10,9],[10,12,10,13],[12,6,12,27],[8,6,8,27]]}
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,"Defect - Damage Monitoring Sheet"]
[]
[null,null,null,null,null,null,null,"Date of Report","01-Jul-2025",null,null,"Ship Name","DHT JAGUAR (03-05-2025)"]
[]
[null,null,null,null,null,null,"VERSION : 2.0"]
[]
[]
[]
[null,null,null,"ID","SHIPSIDE UNIQUEID","UNIQUE ID","Date Recorded","Type of Deficiency","Observer code","Type of Inspection","Description of Deficiency","Equipment Categories","Area of Observation","Deficiency Cause","VIQ Ref Number","Risk Value of Obs","PSC Ref Number","PSC MOU ID","Action Taken or Required","Target Date","PO Ref No.","Status Code","Date Completed","Drydock","Info Sharing","Critical Item","Audit Type","Superintendent Remarks"]
[null,null,null,9352,null,"30_02/01/2020 1:20:51 PM","2018-12-26T23:59:35","Non Conformity","Ship Staff","Ship Staff Insp.","Speed log feed missing from Radar, ECDIS and Log Repeater","Navigation - Echo Sounder / Speed Log","Navigation","Equipment Related","4.7","High","","","Office informed. Awaiting Spares/Technician. Risk Assessment carried out. All Bridge members instructed to use RADAR and ECDIS where the speed log feed is available.   RADAR plotting sheets to be used for collision avoidance. V-DJAG023292/20","2019-02-03T23:59:35","","Completed","2019-02-01T23:59:35","No","No","No","Internal"]
[null,null,null,329,null,"30_Mon Oct 07 2019 09:36:16 GMT+0000","2018-12-27T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Deck projector light fail to switch off","Miscellaneous","General Appearance","Equipment Related","11.9","Low","","","Outdoor relay box renewed with new spare","2019-02-21T23:59:35","DJAG190005","Completed","2019-05-11T23:59:35","No","No","No","Internal"]
[null,null,null,277,null,"30_Sun Oct 06 2019 22:12:29 GMT+0000","2019-01-12T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Composite Boiler steam stop valve bonnet gasket leaking.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.2","Low","","","Need to isolate the boiler derpressurize and change the gasket. V-DJAG023517/20","2019-01-12T23:59:35","","Completed","2019-01-12T23:59:35","No","No","No","Internal"]
[null,null,null,283,null,"30_Sun Oct 06 2019 22:32:41 GMT+0000","2019-01-17T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Turbine ballast pump steam stop valve gland leaking.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","10.32","Very High","","","Isolate the turbine and system and renew the gland.","2019-01-21T23:59:35","","Completed","2019-01-22T23:59:35","No","No","No","Internal"]
[null,null,null,286,null,"30_Sun Oct 06 2019 22:38:47 GMT+0000","2019-01-17T23:59:35","Defect","Ship Staff","Ship Staff Insp.","1 NO. UTI NOT WORKING","Miscellaneous","Cargo / Ballast Systems","Equipment Related","8.12","Medium","","","Require Replacement.","2019-02-01T23:59:35","DJAG190019","Completed","2019-02-03T23:59:35","No","No","No","Internal"]
[null,null,null,287,null,"30_Sun Oct 06 2019 22:40:49 GMT+0000","2019-01-17T23:59:35","Defect","Ship Staff","Ship Staff Insp.","BWTS MONITOR NOT WORKING","Miscellaneous","Cargo / Ballast Systems","Equipment Related","8.8","Medium","","","Awaiting Replacement.","2019-02-01T23:59:35","DJAG190031","Completed","2019-02-03T23:59:35","No","No","No","Internal"]
[null,null,null,279,null,"30_Mon Jun 10 2019 22:20:02 GMT+0000","2019-01-18T23:59:35","Defect","Ship Staff","Ship Staff Insp.","# 1 Main boiler steam stop valve gland leaking.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Need to isolate the boiler derpressurize and change the gland packings. V-DJAG023517/20","2019-01-21T23:59:35","","Completed","2019-01-21T23:59:35","No","No","No","Internal"]
[null,null,null,280,null,"30_Sun Oct 06 2019 22:22:18 GMT+0000","2019-01-19T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Engine room bilge circulating pump losing suction","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","6.15","High","","","Pump to isolate and open the suction/discharge valve overhaul and boxback. V-DJAG023517/20","2019-01-19T23:59:35","","Completed","2019-01-19T23:59:35","No","No","No","Internal"]
[null,null,null,282,null,"30_Sun Oct 06 2019 22:29:22 GMT+0000","2019-01-23T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Fwd Hydraulic motor S.W cooling pipe found with Pin Hole","Deck - Pipe / Fittings","Mooring","Equipment Related","11.12","Low","","","Pipe to be removed and welding to be done in Engine room workshop.","2019-01-24T23:59:35","","Completed","2019-01-23T23:59:35","No","No","No","Internal"]
[null,null,null,288,null,"30_Sun Oct 06 2019 22:43:26 GMT+0000","2019-01-26T23:59:35","Defect","Ship Staff","Ship Staff Insp.","SECURING ARRANGEMENT FOR ELEVATOR DOORS IN ENGINE ROOM IS NOT AVAILABLE. ( IN VIEW OF PIRATE ATTACK )","Miscellaneous","Eng. / Strg. Comp.","External Factors","7.4","Low","","","SECURING ARRANGEMENT TO FABRICATE FOR LOCKING THE HANDLE OF ELEVATOR DOORS IN 2ND & 3RD  DECK IN ENGINE ROOM. V-DJAG023520/20","2019-02-10T23:59:35","","Completed","2019-02-10T23:59:35","No","No","No","Internal"]
[null,null,null,293,null,"30_Sun Oct 06 2019 22:53:17 GMT+0000","2019-02-02T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Fwd Fire Wire Winch - Lack of maintenance & already rusting.","Deck - Mooring Machinery","General Appearance","Equipment Related","9.14","Medium","","","Derusting & Painting of Fwd Fire Wire Winch Carried out. V-DJAG023288/20","2019-04-01T23:59:35","","Completed","2019-02-06T23:59:35","No","No","No","Internal"]
[null,null,null,294,null,"30_Sun Oct 06 2019 22:54:51 GMT+0000","2019-02-02T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","E/R Fans Mushroom Vent Heads - De-rusting required to improve appearance of Engine Casing.","E/R - Pipes/ valves & fittings","General Appearance","External Factors","11.8","Low","","","De-rusting & Painting of E/R Fans Mushroom Vent heads Carried out. V-DJAG023525/20","2019-04-01T23:59:35","","Completed","2019-02-15T23:59:35","No","No","No","Internal"]
[null,null,null,307,null,"30_Sun Oct 06 2019 23:58:59 GMT+0000","2019-02-02T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Main Deck Flood Lighting Lamp Post - Rust stain appearing at the top of the lamp post and also all the flood lighting supports.","Deck - Pipe / Fittings","General Appearance","External Factors","11.1","High","","","Derusting and painting carried out. V-DJAG023289/20","2019-04-01T23:59:35","","Completed","2019-03-27T23:59:35","No","No","No","Internal"]
[null,null,null,302,null,"30_Sun Oct 06 2019 23:14:18 GMT+0000","2019-02-03T23:59:35","Defect","Ship Staff","Ship Staff Insp.","SUNKEN DECK TOILET NOT WORKING.","Accommodation","General Appearance","Equipment Related","11.13","Low","","","SUSPECT MALFUNCTION OF DISCHARGE VALVE,NEED TO ATTEMPT THE JOB.","2019-03-03T23:59:35","","Completed","2019-02-26T23:59:35","No","No","No","Internal"]
[null,null,null,284,null,"30_Sun Oct 06 2019 22:34:29 GMT+0000","2019-02-04T23:59:35","Defect","Ship Staff","Ship Staff Insp.","FUEL OIL STEAM TRACING LINE LEAKING","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Need to isolate and rectify the same. V-DJAG023518/20","2019-02-04T23:59:35","","Completed","2019-02-04T23:59:35","No","No","No","Internal"]
[null,null,null,9353,null,"30_02/01/2020 1:22:56 PM","2019-02-04T23:59:35","Non Conformity","Ship Staff","Ship Staff Insp.","Vessel does not have latest edition of Conoslidated Marpol and STCW 2017 Edition.","Documentation","Navigation","Human Error","4.1","High","","","New editions for Consolidated Marpol and STCW installed and Unlock Key from the service provider ordered for the same.","2019-02-21T23:59:35","","Completed","2019-03-02T23:59:35","No","No","No","Internal"]
[null,null,null,285,null,"30_Sun Oct 06 2019 22:36:23 GMT+0000","2019-02-05T23:59:35","Defect","Ship Staff","Ship Staff Insp.","HFO SETTLING TANK HEATING STEAM INLET FLANGE LEAKING.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Isolate and change the Gasket. V-DJAG023519/20","2019-02-05T23:59:35","","Completed","2019-02-05T23:59:35","No","No","No","Internal"]
[null,null,null,9354,null,"30_02/01/2020 1:25:09 PM","2019-02-09T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Crew documents/Certificates File was not maintained as per Company standard Certificate and documents Index.","Documentation","Cert. & Docu.","Human Error,Knowledge Based","3.6","High","","","Index for all crews file as per Rank was made, all crew documents file were updated as per Index and same index placed in front page of file.","2019-02-13T23:59:35","","Completed","2019-02-12T23:59:35","No","No","No","Internal"]
[null,null,null,289,null,"30_Sun Oct 06 2019 22:45:11 GMT+0000","2019-02-11T23:59:35","Defect","Ship Staff","Ship Staff Insp.","BOILER HEATING LINE RETURN LEAKING NEAR STEAM TRAP.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","STEAM TO ISOLATE AND RECTIFY THE SAME. V-DJAG023521/20","2019-02-11T23:59:35","","Completed","2019-02-11T23:59:35","No","No","No","Internal"]
[null,null,null,292,null,"30_Sun Oct 06 2019 22:50:31 GMT+0000","2019-02-13T23:59:35","Defect","Ship Staff","Ship Staff Insp.","JACKET WATER TEMPERATURE CONTROLLER PNEUMATIC VALVE MALFUNCTION.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","NEED TO CALIBRATE AND CHECK THE PID CONTROLLER AND IF NOT CHANGE WITH THE SPARE ONE AVAILABLE. V-DJAG023524/20","2019-02-13T23:59:35","","Completed","2019-02-13T23:59:35","No","No","No","Internal"]
[null,null,null,290,null,"30_Sun Oct 06 2019 22:47:05 GMT+0000","2019-02-14T23:59:35","Defect","Ship Staff","Ship Staff Insp.","MAIN ENGINE PRE-HEATER INWARD GASKET LEAKING.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","NEED TO ISOLATE AND CHANGE THE GASKET. V-DJAG023522/20","2019-02-15T23:59:35","","Completed","2019-02-15T23:59:35","No","No","No","Internal"]
[null,null,null,291,null,"30_Sun Oct 06 2019 22:48:45 GMT+0000","2019-02-17T23:59:35","Defect","Ship Staff","Ship Staff Insp.","# 1 AE # 5 UNIT HIGH PRESSURE PUMP BLOCK O-RING LEAKING.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","ISOLATE THE SYSTEM AND CHANGE THE O-RING V-DJAG023523/20","2019-02-17T23:59:35","","Completed","2019-02-17T23:59:35","No","No","No","Internal"]
[null,null,null,9355,null,"30_02/01/2020 1:27:04 PM","2019-02-21T23:59:35","Non Conformity","Ship Staff","Ship Staff Insp.","ISPS KEY LOG NOT UPDATED","Documentation","ISPS Related","Human Error,Inappropriate Procedure","7.3","Low","","","DURING ROUTINE INSPECTION OF FILES, FOUND OUT THAT ISPS KEY LOG IS NOT UPDATED BY SHIP STAFF. IMMEDIATELY SAME UPDATED.","2019-02-23T23:59:35","","Completed","2019-02-22T23:59:35","No","No","No","Internal"]
[null,null,null,317,null,"30_Mon Oct 07 2019 00:28:25 GMT+0000","2019-02-22T23:59:35","Defect","Ship Staff","Ship Staff Insp.","BWTS Rectifiers A & B tripping on HIGH Current","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.8","Medium","","","Anodes cleaning carried out. System tried out","2019-05-08T23:59:35","DJAG195019","Completed","2019-04-28T23:59:35","No","No","No","Internal"]
[null,null,null,326,null,"30_Mon Oct 07 2019 09:29:39 GMT+0000","2019-02-22T23:59:35","Defect","Ship Staff","Ship Staff Insp.","BWTS Auto backwash filter mal-functioning, no spare onboard","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.8","Medium","","","Bottom bolts renewed, TEFLON on order V-DJAG024661/20","2019-05-21T23:59:35","DJAG190053","Completed","2019-05-18T23:59:35","No","No","No","Internal"]
[null,null,null,327,null,"30_Mon Oct 07 2019 09:31:18 GMT+0000","2019-02-22T23:59:35","Defect","Ship Staff","Ship Staff Insp.","BWTS TRO sensor not displaying any reading","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.8","Medium","","","TRO sensor primed,flow adjusted","2019-05-21T23:59:35","DJAG190053","Completed","2019-04-28T23:59:35","No","No","No","Internal"]
[null,null,null,297,null,"30_Sun Oct 06 2019 22:59:41 GMT+0000","2019-02-24T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Composite boiler steam stop valve gasket leaking.","E/R - Boiler","General Appearance","Equipment Related","10.32","Very High","","","Depressurize the boiler and change the gasket. V-DJAG017396/19","2019-03-06T23:59:35","","Completed","2019-03-06T23:59:35","No","No","No","Internal"]
[null,null,null,295,null,"30_Sun Oct 06 2019 22:56:35 GMT+0000","2019-02-26T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Main engine Lube oil cooler PID control valve not working.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","PID controller tried to reinitiate and not working then the new one installed. V-DJAG023526/20","2019-03-06T23:59:35","","Completed","2019-03-06T23:59:35","No","No","No","Internal"]
[null,null,null,309,null,"30_Mon Oct 07 2019 00:04:00 GMT+0000","2019-02-28T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Fuel filter line steam gasket leaking.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Gasket to change. V-DJAG023527/20","2019-02-28T23:59:35","","Completed","2019-02-28T23:59:35","No","No","No","Internal"]
[null,null,null,296,null,"30_Sun Oct 06 2019 22:58:12 GMT+0000","2019-03-03T23:59:35","Defect","Ship Staff","Ship Staff Insp.","LT fresh water cooler PID control valve not working.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","PID controller tried to reinitiate and not working then the new one installed. V-DJAG023527/20","2019-03-06T23:59:35","","Completed","2019-03-06T23:59:35","No","No","No","Internal"]
[null,null,null,9356,null,"30_02/01/2020 1:28:51 PM","2019-03-03T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Main engine lube oil cooler auto controller valve not working.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","PID controller was checked and tried to calibrate. Found faulty and same was replaced by a spare one onboard. V-DJAG023526/20","2019-03-06T23:59:35","","Completed","2019-03-06T23:59:35","No","No","No","Internal"]
[null,null,null,298,null,"30_Sun Oct 06 2019 23:01:41 GMT+0000","2019-03-05T23:59:35","Defect","Ship Staff","Ship Staff Insp.","# 1 MAC inter cooler gasket and o-ring leaking.","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Isolate and open the cooler and changed with new. V-DJAG023540/20","2019-03-05T23:59:35","","Completed","2019-03-05T23:59:35","No","No","No","Internal"]
[null,null,null,299,null,"30_Sun Oct 06 2019 23:05:28 GMT+0000","2019-03-05T23:59:35","Defect","Ship Staff","Ship Staff Insp.","# 1 AE attached FW pump mech.seal leaking.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Isolate the system and change the seal. V-DJAG023531/20","2019-03-05T23:59:35","","Completed","2019-03-05T23:59:35","No","No","No","Internal"]
[null,null,null,300,null,"30_Sun Oct 06 2019 23:07:05 GMT+0000","2019-03-05T23:59:35","Defect","Ship Staff","Ship Staff Insp.","# 3 AE attached FW pump mech.seal leaking.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Isolate the system and change the seal. V-DJAG023531/20","2019-03-06T23:59:35","","Completed","2019-03-06T23:59:35","No","No","No","Internal"]
[null,null,null,301,null,"30_Sun Oct 06 2019 23:09:43 GMT+0000","2019-03-05T23:59:35","Defect","Ship Staff","Ship Staff Insp.","# 2 AE FW temperature controller valve ( thermostatic ) not working.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Isolate the system and change the thermostatic valve. V-DJAG023532/20","2019-03-05T23:59:35","","Completed","2019-03-05T23:59:35","No","No","No","Internal"]
[null,null,null,306,null,"30_Sun Oct 06 2019 23:54:52 GMT+0000","2019-03-09T23:59:35","Defect","Ship Staff","Ship Staff Insp.","LDCL pump inlet pressure sensor faulty.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Pressure sensor changed with new spare. V-DJAG023533/20","2019-03-09T23:59:35","","Completed","2019-03-09T23:59:35","No","No","No","Internal"]
[null,null,null,303,null,"30_Sun Oct 06 2019 23:17:29 GMT+0000","2019-03-10T23:59:35","Defect","Ship Staff","Ship Staff Insp.","FWG Inlet line temperature gauge malfunctioning. Angle type.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Vessel replaced with the spare. V-DJAG023533/20","2019-03-11T23:59:35","","Completed","2019-03-11T23:59:35","No","No","No","Internal"]
[null,null,null,304,null,"30_Sun Oct 06 2019 23:20:47 GMT+0000","2019-03-10T23:59:35","Defect","Ship Staff","Ship Staff Insp.","# 1 AE air cooler gasket damage.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","AE isolated and air cooler gasket replaced. V-DJAG023514/20","2019-03-11T23:59:35","","Completed","2019-03-11T23:59:35","No","No","No","Internal"]
[null,null,null,305,null,"30_Sun Oct 06 2019 23:24:52 GMT+0000","2019-03-18T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Sundry fan belt damaged.","","General Appearance","Equipment Related","11.13","Low","","","Fan belt changed with new spare.","2019-03-19T23:59:35","","Completed","2019-03-19T23:59:35","No","No","No","Internal"]
[null,null,null,308,null,"30_Mon Oct 07 2019 00:01:29 GMT+0000","2019-03-29T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Sludge pump gland leaking.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Gland packing to renew. V-DJAG023507/20","2019-03-30T23:59:35","","Completed","2019-03-30T23:59:35","No","No","No","Internal"]
[null,null,null,310,null,"30_Mon Oct 07 2019 00:06:05 GMT+0000","2019-04-02T23:59:35","Defect","Ship Staff","Ship Staff Insp.","AE turbocharger air cooler inlet line to air cooler leaking.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Gasket to renew. V-DJAG023469/20","2019-04-02T23:59:35","","Completed","2019-04-02T23:59:35","No","No","No","Internal"]
[null,null,null,350,null,"30_Mon Oct 07 2019 10:17:44 GMT+0000","2019-04-04T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Boiler fuel oil burning pump mech. seal leaking.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Mech seal to be renewed. Pump dismantled seal surface cleaned.RO raised. Found spare seal onboard. Replaced and no leak from Seal V-DJAG023469/20","2019-05-13T23:59:35","DJAG190062","Completed","2019-07-14T23:59:35","No","No","No","Internal"]
[null,null,null,311,null,"30_Mon Oct 07 2019 00:08:06 GMT+0000","2019-04-07T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Boiler fuel oil heater steam inlet line flange leaking.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Gasket to renew. V-DJAG023479/20","2019-04-07T23:59:35","","Completed","2019-04-07T23:59:35","No","No","No","Internal"]
[null,null,null,330,null,"30_Mon Oct 07 2019 09:39:05 GMT+0000","2019-04-10T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Mooring tails 7 Nos. got expired on 18th March 2019.  Requisition raised for the same on 16-Jan-2019.","Deck - Mooring Machinery","Mooring","Equipment Related","9.4","High","","","New mooring tails rcvd and same replaced V-DJAG023293/20","2019-05-13T23:59:35","DJAG190018","Completed","2019-05-23T23:59:35","No","No","No","Internal"]
[null,null,null,312,null,"30_Mon Oct 07 2019 00:10:57 GMT+0000","2019-04-13T23:59:35","Defect","Ship Staff","Ship Staff Insp.","ME fuel oil back wash filter o-ring leaking.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Filter isolated and renewed with new o-ring. V-DJAG023535/20","2019-04-13T23:59:35","","Completed","2019-04-13T23:59:35","No","No","No","Internal"]
[null,null,null,313,null,"30_Mon Oct 07 2019 00:13:05 GMT+0000","2019-04-13T23:59:35","Defect","Ship Staff","Ship Staff Insp.","AE # 1 Fuel link leaking.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","AE to isolate and lekaing o-rings replaced.","2019-04-13T23:59:35","","Completed","2019-04-13T23:59:35","No","No","No","Internal"]
[null,null,null,314,null,"30_Mon Oct 07 2019 00:16:48 GMT+0000","2019-04-15T23:59:35","Defect","Ship Staff","Ship Staff Insp.","AE fuel oil back wash filter o-ring leaking.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Filter isolated and renewed with new o-ring. V-DJAG023478/20","2019-04-15T23:59:35","","Completed","2019-04-15T23:59:35","No","No","No","Internal"]
[null,null,null,318,null,"30_Mon Oct 07 2019 00:32:14 GMT+0000","2019-04-15T23:59:35","Defect","Ship Staff","Ship Staff Insp.","# 1 ECR cooler suction pressure gauge faulty and leaking.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Spare ordered and same isolated for the time being. V-DJAG023477/20","2019-05-08T23:59:35","DJAG190060","Completed","2019-05-12T23:59:35","No","No","No","Internal"]
[null,null,null,315,null,"30_Mon Oct 07 2019 00:21:32 GMT+0000","2019-04-16T23:59:35","Defect","Ship Staff","Ship Staff Insp.","# 1 Fire & GS pump mech.seal leaking.","E/R - Pumps","Safety / LSA / FFA","Equipment Related","10.31","Very High","","","Pump isolated and mech.seal changed.","2019-04-17T23:59:35","","Completed","2019-04-17T23:59:35","No","No","No","Internal"]
[null,null,null,9357,null,"30_02/01/2020 1:30:35 PM","2019-04-17T23:59:35","Non Conformity","Ship Staff","Ship Staff Insp.","7 Nos. of Mooring tails got expired on 18 march 2019, requistion for the same has been raised. vessel awaiting supply.","Miscellaneous","Mooring","Equipment Related","9.17","High","","","requisition raised for the same, awaiting for suppy. Office informed and  expired mooring tails inspected and elongation test carried out for the same. V-DJAG023293/20","2019-06-23T23:59:35","","Completed","2019-05-23T23:59:35","No","No","No","Internal"]
[null,null,null,316,null,"30_Mon Oct 07 2019 00:24:32 GMT+0000","2019-04-19T23:59:35","Defect","Ship Staff","Ship Staff Insp.","FWD & AFT LT cooler sacrificial flange leaking.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","LT coolers isolated and flanges changed with new spare.","2019-04-19T23:59:35","","Completed","2019-04-19T23:59:35","No","No","No","Internal"]
[null,null,null,7281,null,"30_Fri Dec 06 2019 09:26:22 GMT+0000 (Coordinated Universal Time)","2019-04-24T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Mooring Audit","Anti skid surface below mooring winches barrel appear to have disappeared -  to repaint","Miscellaneous","Mooring","External Factors","9.13","Low","","","All mooring winch area inspected and anti skid area re-painted as required. V-DJAG023312/20","2019-06-24T23:59:35","","Completed","2019-05-21T23:59:35","No","No","No","Internal"]
[null,null,null,7282,null,"30_Fri Dec 06 2019 09:36:54 GMT+0000 (Coordinated Universal Time)","2019-04-24T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Others (Eg. Insurance etc.)","P/R entrance - portable gas meter is lying on deck. This is an expensive critical equipment. To fabricate a wooden stand / box between cables for gas meter to be checked at a working level.","Miscellaneous","Cargo / Ballast Systems","Human Error,Industry Issue,Knowledge Based","5.23","Very High","","","Wooden box fabricated for gas meters on pumproom top to check the gases at working level. V-DJAG023313/20","2019-06-24T23:59:35","","Completed","2019-05-01T23:59:35","No","No","No","Internal"]
[null,null,null,7283,null,"30_Fri Dec 06 2019 09:42:57 GMT+0000 (Coordinated Universal Time)","2019-04-24T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Others (Eg. Insurance etc.)","P/R bottom looks pretty - but the ballast pump strainers can do with a fresh coat of paint ","Miscellaneous","Cargo / Ballast Systems","Equipment Related,Industry Issue","8.8","Medium","","","Water ballast pump strainers painted. V-DJAG023314/20","2019-06-24T23:59:35","","Completed","2019-05-02T23:59:35","No","No","No","Internal"]
[null,null,null,7284,null,"30_Fri Dec 06 2019 09:48:24 GMT+0000 (Coordinated Universal Time)","2019-04-24T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Engineering Audit","E/R emergency bilge suction - lashing wheel with railing is not full proof as it can be bypassed. recommend use the hole provided on valve spindle to pass the numbered cable tie to make it FULL PROOF","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Inappropriate Procedure","6.15","High","","","Sealed immediately put on the valve spindle and ships staff made aware. V-DJAG023225/20","2019-05-24T23:59:35","","Completed","2019-04-25T23:59:35","No","No","No","Internal"]
[null,null,null,7285,null,"30_Wed Jun 12 2019 09:52:23 GMT+0000 (Coordinated Universal Time)","2019-04-24T23:59:35","Defect","Owner / Marine / Tech. Suptd.","ISPS Audit","Briefing as per g'way template was not carried out with SIRE inspector as well as DPA upon boarding at Dong Jia  Kaou berth ","Miscellaneous","ISPS Related","Behaviour Based,Human Error","7.12","High","","","All crew members briefed with importance & consequence to not carrying out proper breifing for visitors on ship.\n\nA gangway breifing tempelate is readily available at gangway & same to be used for breifing the visitors boarding the vessel.\n\n","2019-05-24T23:59:35","","Completed","2019-05-18T23:59:35","No","No","No","Internal"]
[null,null,null,7286,null,"30_Fri Dec 06 2019 09:55:22 GMT+0000 (Coordinated Universal Time)","2019-04-24T23:59:35","Defect","Owner / Marine / Tech. Suptd.","ISM Audit","Port anchor - Guillotine bar does not rest flush on open link   ","Deck - Machinery","ISM Related","Equipment Related,External Factors","9.2","Very High","","","Anchor twist taken out at safe anchorage port suez. V-DJAG023315/20","2019-09-24T23:59:35","","Completed","2019-05-30T23:59:35","No","No","No","Internal"]
[null,null,null,7287,null,"30_Fri Dec 06 2019 10:01:16 GMT+0000 (Coordinated Universal Time)","2019-04-24T23:59:35","Defect","Owner / Marine / Tech. Suptd.","ISM Audit","New set of deck & engine log books were not yet received by the vessel - upon receipt in S'pore to switch to using same asap.","Miscellaneous","ISM Related","External Factors","4.2","Medium","","","Rcvd New log book and started using. V-DJAG023317/20","2019-05-24T23:59:35","","Completed","2019-05-21T23:59:35","No","No","No","Internal"]
[null,null,null,7288,null,"30_Wed Jun 12 2019 10:05:57 GMT+0000 (Coordinated Universal Time)","2019-04-24T23:59:35","Defect","Owner / Marine / Tech. Suptd.","MLC Audit","Rounds of accommodation was not undertaken by Master  - it was being carried out by Ch.off only","","MLC Related","Human Error","11.13","Low","","","Accommodation inspection to be carried out weekly by Master, C/O, C/E & Bosun for proper cleaning and hygiene.","2019-05-24T23:59:35","","Completed","2019-05-19T23:59:35","No","No","No","Internal"]
[null,null,null,319,null,"30_Mon Oct 07 2019 01:06:22 GMT+0000","2019-05-09T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Oxy-Acetylene Bottle Room fixed pipe is not painted BLUE and RED respectively.","E/R - Pipes/ valves & fittings","General Appearance","External Factors","5.26","Medium","","","Pipes painted V-DJAG023585/20","2019-05-09T23:59:35","","Completed","2019-05-09T23:59:35","No","No","No","Internal"]
[null,null,null,320,null,"30_Mon Oct 07 2019 04:36:10 GMT+0000","2019-05-09T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ME turbochargers filters dirty","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.3","Medium","","","Filters renewed V-DJAG023476/20","2019-05-09T23:59:35","","Completed","2019-05-09T23:59:35","No","No","No","Internal"]
[null,null,null,321,null,"30_Mon Oct 07 2019 04:45:38 GMT+0000","2019-05-09T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","DG turbocharger filters dirty","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.3","Medium","","","Filters renewed V-DJAG023474/20","2019-05-09T23:59:35","","Completed","2019-05-09T23:59:35","No","No","No","Internal"]
[null,null,null,322,null,"30_Mon Oct 07 2019 09:12:15 GMT+0000","2019-05-09T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Main Engine Fuel Valve spare parts inventory is not up-dated with actual ROB.","Miscellaneous","General Appearance","Equipment Related","10.13","Very High","","","Inventory updated in PAL","2019-05-16T23:59:35","","Completed","2019-05-12T23:59:35","No","No","No","Internal"]
[null,null,null,323,null,"30_Mon Oct 07 2019 09:14:37 GMT+0000","2019-05-09T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Officers’ Recreation Room, oil stained foot prints on the carpet to clean off.","Accommodation","General Appearance","Human Error","11.13","Low","","","Carpet cleaning carried out V-DJAG023290/20","2019-05-16T23:59:35","","Completed","2019-05-12T23:59:35","No","No","No","Internal"]
[null,null,null,324,null,"30_Mon Oct 07 2019 09:25:09 GMT+0000","2019-05-09T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Some of the Life Buoy Ring grab lines are not as per SOLAS.","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.31","High","","","All grab lines renewed with new one received at Singapore","2019-07-09T23:59:35","","Completed","2019-06-06T23:59:35","No","No","No","Internal"]
[null,null,null,331,null,"30_Mon Oct 07 2019 09:43:37 GMT+0000","2019-05-09T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Engine Casing port side ‘Tiger Stripe’ stains, need a new coat of white paint.","Hull & Tanks","General Appearance","Equipment Related","11.1","High","","","Stains washed & re-coated with a new coat of white paint","2019-07-09T23:59:35","","Completed","2019-05-25T23:59:35","No","No","No","Internal"]
[null,null,null,332,null,"30_Mon Oct 07 2019 09:46:17 GMT+0000","2019-05-09T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","E/R No.1,2,3 and 4 Supply Fan fire damper air cylinder box  is rusting.","Deck - Pipe / Fittings","General Appearance","External Factors","11.1","High","","","De-rusted & Painted","2019-07-09T23:59:35","","Completed","2019-05-28T23:59:35","No","No","No","Internal"]
[null,null,null,333,null,"30_Mon Oct 07 2019 09:48:14 GMT+0000","2019-05-09T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","P & S Life Boat canopy has discoloured.","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.29","High","","","Washed thoroughly both L/B canopy at anchorage V-DJAG023294/20","2019-07-09T23:59:35","","Completed","2019-06-06T23:59:35","No","No","No","Internal"]
[null,null,null,334,null,"30_Mon Oct 07 2019 09:50:33 GMT+0000","2019-05-09T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Em DG Room Aft Exh Fan mushroom vent head is rusting","Miscellaneous","General Appearance","External Factors","11.3","Medium","","","De-rusted & Painted","2019-07-09T23:59:35","","Completed","2019-05-25T23:59:35","No","No","No","Internal"]
[null,null,null,335,null,"30_Mon Oct 07 2019 09:52:49 GMT+0000","2019-05-09T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","No.2S HFO Tank aft vent head is rusting.","Hull & Tanks","General Appearance","External Factors","11.7","High","","","De-rusted & Painted","2019-06-09T23:59:35","","Completed","2019-05-25T23:59:35","No","No","No","Internal"]
[null,null,null,338,null,"30_Mon Oct 07 2019 09:57:38 GMT+0000","2019-05-09T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Radar Mast to de-rust and paint.","Hull & Tanks","General Appearance","External Factors","11.8","Low","","","Spot derusting & painting carried out. V-DJAG023296/20","2019-07-09T23:59:35","","Completed","2019-06-10T23:59:35","No","No","No","Internal"]
[null,null,null,9358,null,"30_02/01/2020 1:32:18 PM","2019-05-15T23:59:35","Observation","Ship Staff","Ship Staff Insp.","It was reported by Bosun that pneumatic needle gun trigger found secured by tape during inspection.","Miscellaneous","ISM Related","Equipment Related","5.11","Low","","","Immediately the tape was removed & all crew briefed about the hazards of trigger kept secured.","2019-05-16T23:59:35","","Completed","2019-05-15T23:59:35","No","No","No","Internal"]
[null,null,null,325,null,"30_Mon Oct 07 2019 09:27:02 GMT+0000","2019-05-17T23:59:35","Defect","Ship Staff","Ship Staff Insp.","FWG flowmeter not operational","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","flowmeter renewed with new spare","2019-05-22T23:59:35","","Completed","2019-05-18T23:59:35","No","No","No","Internal"]
[null,null,null,371,null,"30_Mon Oct 07 2019 10:48:24 GMT+0000","2019-05-17T23:59:35","Defect","Ship Staff","Ship Staff Insp.","One newly received multigas meter not working.","Cargo Mach.,LSA / FFA","Cargo / Ballast Systems","Equipment Related","5.23","Very High","","","Received new gas meter ay Yeosu, South Korea V-DJAG023309/20","2019-06-09T23:59:35","","Completed","2019-09-09T23:59:35","No","No","No","Internal"]
[null,null,null,343,null,"30_Mon Oct 07 2019 10:06:52 GMT+0000","2019-05-22T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Gas bottle for calibration of fixed gas detection system expired.","Cargo Mach.","Cargo / Ballast Systems","Human Error","8.46","Very High","","","Received at GOLA on 15 JULY 2019 V-DJAG023298/20","2019-06-09T23:59:35","DJAG190105","Completed","2019-07-08T23:59:35","No","No","No","Internal"]
[null,null,null,336,null,"30_Mon Oct 07 2019 09:54:26 GMT+0000","2019-05-27T23:59:35","Defect","Ship Staff","Ship Staff Insp.","No.1 & 2 Fire/Foam isolation valve on deck difficult to operate by hand. To be eased & greased.","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.38","High","","","Both valves greased & eased for freedom of movement by hand V-DJAG023295/20","2019-05-30T23:59:35","","Completed","2019-05-28T23:59:35","No","No","No","Internal"]
[null,null,null,5692,null,"30_15/10/2019 10:34:09 AM","2019-05-30T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Stbd Boiler Bellow damaged, require replacement","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Spares received on 13 Sep. 2019 , Bellow replaced V-DJAG023284/20","2019-10-13T23:59:35","DJAG190063","Completed","2019-10-09T23:59:35","No","No","No","Internal"]
[null,null,null,5694,null,"30_15/10/2019 10:30:55 AM","2019-05-30T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Port Side Boiler Exhaust Bellow leaking","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Bellow to replace on receipt. Spares received on 16th Sep. 2019. Replaced Bellow with new. System Tried out. All satisfactory. V-DJAG023283/20","2019-10-18T23:59:35","DJAG190063","Completed","2019-10-04T23:59:35","No","No","No","Internal"]
[null,null,null,340,null,"30_Mon Oct 07 2019 10:01:19 GMT+0000","2019-05-30T23:59:35","Defect","Ship Staff","Ship Staff Insp.","BWTS for Unit #2 not working, Sensor faulty, To replace on receipt","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.8","Medium","","","Requisition raised, to replace on receipt. Repaired onboard and system checked, satisfactory. V-DJAG024659/20","2019-07-13T23:59:35","DIAG190053","Completed","2019-06-25T23:59:35","No","No","No","Internal"]
[null,null,null,351,null,"30_Mon Oct 07 2019 10:19:50 GMT+0000","2019-05-30T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Aft Peak Tank BWTS not working, Solenoide canbalised to Main BWPTS, To replace on receipt","Cargo Mach.","Eng. / Strg. Comp.","Equipment Related","8.8","Medium","","","Requisition raised, to replace on receipt. System tried out by repairing old intake assembly. All working satisfactory. V-DJAG023473/20","2019-07-13T23:59:35","DIAG190095","Completed","2019-08-06T23:59:35","No","No","No","Internal"]
[null,null,null,352,null,"30_Mon Oct 07 2019 10:21:28 GMT+0000","2019-05-30T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Noticed Pick sensor A failure alarm blocked on MOP, after deblocking noticed alarm appears during excessive vibration while running of main Engine","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Suspect loose Electric connections, office informed and to indentify cause in progress. Found damaged cable of Encoder A near Encoder,. Cable repaired by insulation tape. No alram on system. V-DJAG023583/20","2019-09-23T23:59:35","","Completed","2019-08-02T23:59:35","No","No","No","Internal"]
[null,null,null,353,null,"30_Mon Oct 07 2019 10:22:38 GMT+0000","2019-05-30T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Noticed Low Insulation Alarm of ECS manually cut out at MOP","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.38","Medium","","","Alram appearing for friction of seconds during running of engine and almost at every one second interval. Office informed. Low insulation was from damaged Encoder cable near Encoder, same repaired V-DJAG020956/19","2019-09-23T23:59:35","","Completed","2019-08-02T23:59:35","No","No","No","Internal"]
[null,null,null,355,null,"30_Mon Oct 07 2019 10:25:23 GMT+0000","2019-05-30T23:59:35","Defect","Ship Staff","Ship Staff Insp.","AC Compressor #1 found to be less effective","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Opened up Unit, Found 33% load mechanism not working, 100% unit port side vv plate broken and cap. Control mechanism pin damaged and out. Removed all unmit liners and repaired all. Unit Tried out, Performance satisfactory. V-DJAG023465/20","2019-08-24T23:59:35","","Completed","2019-08-05T23:59:35","No","No","No","Internal"]
[null,null,null,359,null,"30_Mon Oct 07 2019 10:31:24 GMT+0000","2019-05-30T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Notice AC Compressor low performance, Capacity Control mechanism malfunctioning, Less gas in system","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Compressor opened up and found damaged Valve plate, liner sealing and piston top of 100% load inner piston. 33% load mechanism connections out. All repairs carried out, replaced valve plate, Oil. Charged about 52 Kgs of Gas. System tried out, performance satisfactory. V-DJAG023465/20","2019-08-24T23:59:35","","Completed","2019-08-09T23:59:35","No","No","No","Internal"]
[null,null,null,364,null,"30_Mon Oct 07 2019 10:38:02 GMT+0000","2019-05-30T23:59:35","Defect","Ship Staff","Ship Staff Insp.","UPS for Citadel not working. System going on bypass mode. Automation system abnormal.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","11.1","High","","","Office informed and maker's advice sought. Job planned to be undertaken By service Engineer in Korea on 13th Sep. 2019. Job attended by service engineer and rectified the defect. V-DJAG021443/19","2019-10-08T23:59:35","DJAG195045","Completed","2019-09-10T23:59:35","No","No","No","Internal"]
[null,null,null,365,null,"30_Mon Oct 07 2019 10:39:31 GMT+0000","2019-05-30T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Exhaust Line Bypass valve in operative","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Found valve alarm on MOP manually reposed and valve positioner locally kept on manual mode. Calibrated the positioner checked operation, valve founnd to be operating. Later checked operation from MOP , noticed valve is working. Further during sailing noticed sometime valves taking longer time to close, that can be due to Carbon deposits inside valve seat or Air Actuator not able to Force shut the valve due to leaking seal rings. Job of overhauling the valve to be undertaken during ME stoppage . Valve Positioner feed back unit replaced. Performance satisfactory V-DJAG023462/20","2019-09-23T23:59:35","","Completed","2019-09-07T23:59:35","No","No","No","Internal"]
[null,null,null,372,null,"30_Mon Oct 07 2019 10:50:24 GMT+0000","2019-05-30T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Elevator Timer Relay for Control panel defective","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.37","Medium","","","Requisition raised, to replace on receipt V-DJAG023200/20","2019-08-24T23:59:35","DJAG190067","Completed","2019-09-14T23:59:35","No","No","No","Internal"]
[null,null,null,270,null,"30_Wed Jul 10 2019 10:56:52 GMT+0000","2019-06-03T23:59:35","Defect","Ship Staff","Ship Staff Insp.","HFO Purifier #2 Sealing water Non Return Valve not holding, damaged","E/R - Purifier","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Waiting for Spares. Spares Received on 03rd Oct. 2019 V-DJAG023201/20","2019-09-23T23:59:35","DJAG190112","Completed","2019-10-05T23:59:35","No","No","No","Internal"]
[null,null,null,337,null,"30_Mon Oct 07 2019 09:56:04 GMT+0000","2019-06-04T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Service Air Compressor Air Outlet NRV not holding","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Overhauled with new Spring, System working satisfactory","2019-06-05T23:59:35","","Completed","2019-06-05T23:59:35","No","No","No","Internal"]
[null,null,null,373,null,"30_Mon Oct 07 2019 10:52:04 GMT+0000","2019-06-04T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Incinerator Combustion Air Switch Faulty","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Awaiting for Spares. to be rectified. V-DJAG023201/20","2019-07-08T23:59:35","DJAG190047","Completed","2019-08-14T23:59:35","No","No","No","Internal"]
[null,null,null,339,null,"30_Mon Oct 07 2019 09:59:26 GMT+0000","2019-06-11T23:59:35","Defect","Ship Staff","Ship Staff Insp.","1P WBT stbd gas sampling point pipe near inlet valve bent.","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","External Factors","11.4","Very High","","","Pipe disconnected, straightened & fitted back. V-DJAG023297/20","2019-06-23T23:59:35","","Completed","2019-06-20T23:59:35","No","No","No","Internal"]
[null,null,null,9359,null,"30_02/01/2020 1:33:53 PM","2019-06-16T23:59:35","Non Conformity","Ship Staff","Ship Staff Insp.","Few visitor cards found missing","Documentation","ISPS Related","Human Error","7.12","High","","","Office informed about the missing visitor cards. All ship staff to be trained to verify all visitors hand over their respective cards prior disembarkation. Same to be verified after deprture each port of call by SSO.","2019-09-16T23:59:35","","Completed","2019-07-20T23:59:35","No","No","No","Internal"]
[null,null,null,344,null,"30_Mon Oct 07 2019 10:08:46 GMT+0000","2019-06-21T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Mechanical damage caused due to mooring wires on main deck in few areas.","Hull & Tanks","General Appearance","External Factors","9.18","Low","","","Spot maintenance & painting carried out. V-DJAG023299/20","2019-06-28T23:59:35","","Completed","2019-06-27T23:59:35","No","No","No","Internal"]
[null,null,null,342,null,"30_Mon Oct 07 2019 10:04:21 GMT+0000","2019-06-24T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Positioner for ME Jacket water Temperature controller not operating","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Attempted with calibration for old positioner. Later Replaced with new spare onboard and calibrated. V-DJAG023584/20","2019-07-04T23:59:35","","Completed","2019-07-04T23:59:35","No","No","No","Internal"]
[null,null,null,341,null,"30_Mon Oct 07 2019 10:02:52 GMT+0000","2019-07-02T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Elevator not stopping at bottom Deck and Down limit stop  alram coming","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","11.1","High","","","Checked and found bottom slow down limit switch was not alligned, so no operating. Same alligned and system made operational. V-DJAG020187/19","2019-07-02T23:59:35","","Completed","2019-07-02T23:59:35","No","No","No","Internal"]
[null,null,null,345,null,"30_Mon Oct 07 2019 10:10:24 GMT+0000","2019-07-05T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Gyro display Alarm, Actual value found OK without any error","Navigation - Others","Navigation","Equipment Related","4.9","Medium","","","Gyro system switched off completely and restarted after 05 minutes. All Error Alarms disappeared V-DJAG023300/20","2019-07-17T23:59:35","","Completed","2019-07-16T23:59:35","No","No","No","Internal"]
[null,null,null,349,null,"30_Mon Oct 07 2019 10:16:33 GMT+0000","2019-07-07T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Aux. Blower #1 Contactor coil found burnt during routine maintenance","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.3","Medium","","","Replaced with spare coil and system checked for performance. All Satisfactory. V-DJAG023470/20","2019-07-08T23:59:35","","Completed","2019-07-07T23:59:35","No","No","No","Internal"]
[null,null,null,354,null,"30_Mon Oct 07 2019 10:24:07 GMT+0000","2019-07-07T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Conning Unit, AIS alram on ECDIS, Radar and Conning panel","Navigation - ECDIS","Navigation","Equipment Related","4.7","High","","","Changed port of Conning unit and replaced the communication wire. Alarms disappeared from ECDIS #2, Radar and Conning unit panel, but still alarm appears on ECDIS#1 display unit for Conning unit error. Office informed, fault finding in progress. Replaced communication cable of Conning Unit. all alarm disappeared. V-DJAG023301/20","2019-10-23T23:59:35","","Completed","2019-07-25T23:59:35","No","No","No","Internal"]
[null,null,null,366,null,"30_Mon Oct 07 2019 10:41:00 GMT+0000","2019-07-07T23:59:35","Defect","Ship Staff","Ship Staff Insp.","VDR Float free system Communication Alarm error with Float free EPIRB","Navigation - VDR / BNWAS","Navigation","Equipment Related","4.7","High","","","Checked wiring, Reset/ restarted the system, Checked voltage at local JB (52 Volts). Suspected magnetic base faulty due to lightening. Office informed, Fault finding in progress. Office to raise requisition for spares. Job attended by service engineer. Magnetic base replaced. All faults cleared V-DJAG023304/20","2019-10-23T23:59:35","","Completed","2019-09-11T23:59:35","No","No","No","Internal"]
[null,null,null,367,null,"30_Mon Oct 07 2019 10:42:23 GMT+0000","2019-07-07T23:59:35","Defect","Ship Staff","Ship Staff Insp.","HF/MF unit Failure","Navigation - GMDSS & Communication","Navigation","Equipment Related","4.24","High","","","Able to receive signal, but not able to transmit. Checked two PCB's,  burnt because of lightening, Office informed and requisition raised. Replaced unit on receipt (Tuner Unit). Checked Performance. All Satisfactory. V-DJAG023305/20","2019-10-23T23:59:35","DJAG195041","Completed","2019-08-09T23:59:35","No","No","No","Internal"]
[null,null,null,368,null,"30_Mon Oct 07 2019 10:43:39 GMT+0000","2019-07-07T23:59:35","Defect","Ship Staff","Ship Staff Insp.","IMMARSAT -C #1  showing error,","Navigation - GMDSS & Communication","Navigation","Equipment Related","4.24","High","","","Swapped connection with other Unit, found Bridge unit satisfactory. Suspect Faulty Antenna. Office informed, requisition raised. Replaced Anetena Unit at Yosu Korea. Checked performance, all satisfactory.V-DJAG023306/20","2019-10-23T23:59:35","DJAG190141","Completed","2019-08-09T23:59:35","No","No","No","Internal"]
[null,null,null,369,null,"30_Mon Oct 07 2019 10:44:56 GMT+0000","2019-07-07T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Anemometer Faulty, showing Error","Navigation - Others","Navigation","Equipment Related","4.7","High","","","Found Broken Wind directional and on further investigation suspect PCB defective at main panel due to lightening. Requisition raised for Spares. Replaced spare after receiving at Yosu. Checked Performance. All satisfactory. V-DJAG023307/20","2019-10-23T23:59:35","DJAG190140","Completed","2019-08-09T23:59:35","No","No","No","Internal"]
[null,null,null,346,null,"30_Mon Oct 07 2019 10:11:39 GMT+0000","2019-07-08T23:59:35","Defect","Ship Staff","Ship Staff Insp.","ME Jacket water Temperature controller not responding","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Replaced and calibrated with new onboard Spare. System Checked, working on auto mode V-DJAG023584/20","2019-07-13T23:59:35","","Completed","2019-07-10T23:59:35","No","No","No","Internal"]
[null,null,null,347,null,"30_Mon Oct 07 2019 10:13:49 GMT+0000","2019-07-09T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Found Sacrificial Flange of LT cooler #1 bypass line leaking","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Removed pipeline, noticed previously done job was no carried out properly and due to stresses Joint started leaking. Found damaged gasket and Flange found to be OK. Still replaced with new flange and gasket and leaks eliminated V-DJAG023472/20","2019-07-13T23:59:35","","Completed","2019-07-12T23:59:35","No","No","No","Internal"]
[null,null,null,348,null,"30_Mon Oct 07 2019 10:15:19 GMT+0000","2019-07-13T23:59:35","Defect","Ship Staff","Ship Staff Insp.","During routine inspection found few of FO tank Vent float damaged","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","11.7","High","","","Damaged plastic floats replaced with steel floats. V-DJAG023471/20","2019-07-13T23:59:35","","Completed","2019-07-13T23:59:35","No","No","No","Internal"]
[null,null,null,9360,null,"30_02/01/2020 1:35:27 PM","2019-07-20T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Holes found in Bulk head panellings  in accommodation","Accommodation","General Appearance","Human Error","11.13","Low","","","All Holes sealed with Silicon.","2019-07-20T23:59:35","","Completed","2019-07-20T23:59:35","No","No","No","Internal"]
[null,null,null,271,null,"30_Mon Oct 07 2019 10:59:47 GMT+0000","2019-07-23T23:59:35","Defect","Ship Staff","Ship Staff Insp.","2 nos of FW valves found leaking on deck.","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.4","Very High","","","Spares rcvd and valves renewed. V-DJAG023275/20","2019-09-23T23:59:35","DJAG190153","Completed","2019-10-03T23:59:35","No","No","No","Internal"]
[null,null,null,272,null,"30_Mon Oct 07 2019 11:02:11 GMT+0000","2019-07-26T23:59:35","Defect","Ship Staff","Ship Staff Insp.","ME FO Cir. PP #2 abnormal Sound","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Overhauled Motor on 09th April 2019 and replaced bearings, Noise still appears. Raised requisition to overhaul the pump. Further Lifted up Motor on 22nd Aug. 2019, found damaged Magnets. Damaged parts removed and motor fixed back. noice reduced significantly","2019-09-23T23:59:35","DJAG190119","Completed","2019-10-04T23:59:35","No","No","No","Internal"]
[null,null,null,357,null,"30_Mon Oct 07 2019 10:28:40 GMT+0000","2019-07-26T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Bonding cable of Light fittings missing on many places","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.37","Medium","","","Job started and to complete . V-DJAG023467/20","2019-08-24T23:59:35","","Completed","2019-08-20T23:59:35","No","No","No","Internal"]
[null,null,null,9361,null,"30_02/01/2020 1:38:00 PM","2019-08-01T23:59:35","Observation","Ship Staff","Ship Staff Insp.","NOTICED WATER BOTTLES KEPT BEHIND ELECTRIC PANEL","Miscellaneous","Eng. / Strg. Comp.","Human Error,Knowledge Based","10.29","Medium","","","MMEDIATELY CONCERNED PERSON MADE AWARE OF CONSEQUENCES AND ASKED TO REMOVE WATER BOTTLES","2019-08-23T23:59:35","","Completed","2019-08-01T23:59:35","No","No","No","Internal"]
[null,null,null,356,null,"30_Mon Oct 07 2019 10:26:34 GMT+0000","2019-08-16T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Vacuum Cond. Automatic Control Valve air leaking","Cargo Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Dismantled Valve, found damaged Diaphragm. Doaphragm repaired and leak stopped. Requisition raised for new Diaphragm V-DJAG023582/20","2019-08-16T23:59:35","","Completed","2019-08-16T23:59:35","No","No","No","Internal"]
[null,null,null,358,null,"30_Mon Oct 07 2019 10:30:08 GMT+0000","2019-08-16T23:59:35","Defect","Ship Staff","Ship Staff Insp.","220 Volt Low Insulation","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.38","Medium","","","Found water ingress in thee in No fittings. Two removed and cleaned, Midship Light removed and changed the ignitor. Insulation improved to 5 mehga ohms. V-DJAG023466/20","2019-08-23T23:59:35","","Completed","2019-08-20T23:59:35","No","No","No","Internal"]
[null,null,null,273,null,"30_Mon Oct 07 2019 11:04:29 GMT+0000","2019-08-17T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Found ME preheater Temp gauge, LDL pp dish press. Gauge, 19K dump vv instrument gauge not working. ","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Defective gauges listed replaced and few more gauges found too replaced. V-DJAG023515/20","2019-09-23T23:59:35","DJAG190158","Completed","2019-10-24T23:59:35","No","No","No","Internal"]
[null,null,null,360,null,"30_Mon Oct 07 2019 10:32:33 GMT+0000","2019-08-23T23:59:35","Defect","Ship Staff","Ship Staff Insp.","AE #1 found all Exhaust Temperatures high","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Opened up T/C , found damaged blower impeller and Inlet insert. Replaced T/C with new spare cartridge, Generator tried out, performance satisfactory. V-DJAG023464/20","2019-08-24T23:59:35","","Completed","2019-08-24T23:59:35","No","No","No","Internal"]
[null,null,null,361,null,"30_Mon Oct 07 2019 10:33:52 GMT+0000","2019-08-31T23:59:35","Defect","Ship Staff","Ship Staff Insp.","OverFill alram Light indication not working","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.14","Very High","","","Found PCB not workinhg, Light made operational with one Old PCB","2019-09-03T23:59:35","","Completed","2019-09-03T23:59:35","No","No","No","Internal"]
[null,null,null,362,null,"30_Mon Oct 07 2019 10:35:13 GMT+0000","2019-08-31T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Forepeak Water Ballast Remote gauging system malfunctioning.","Hull & Tanks","Cargo / Ballast Systems","Equipment Related","8.12","Medium","","","Tank opened up and found line chocked, cleared same and system made operational V-DJAG023303/20","2019-08-31T23:59:35","","Completed","2019-08-31T23:59:35","No","No","No","Internal"]
[null,null,null,363,null,"30_Mon Oct 07 2019 10:36:36 GMT+0000","2019-08-31T23:59:35","Defect","Ship Staff","Ship Staff Insp.","LDCL Pump Seal Leaking","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Removed Pump and replaced seal with Spare onboard V-DJAG023463/20","2019-09-06T23:59:35","","Completed","2019-09-06T23:59:35","No","No","No","Internal"]
[null,null,null,370,null,"30_Mon Oct 07 2019 10:46:29 GMT+0000","2019-08-31T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Fwd Windlass controller PLC defective","Deck - Mooring Machinery","Mooring","Equipment Related","9.2","Very High","","","Requisition raised, will replace oin recept, System made operational on Emergency mode. PLC unit changed and system tried out, Performance satisfactory. V-DJAG023199/20","2019-09-23T23:59:35","DJAG190178","Completed","2019-09-12T23:59:35","No","No","No","Internal"]
[null,null,null,7289,null,"30_Fri Dec 06 2019 10:48:24 GMT+0000 (Coordinated Universal Time)","2019-09-10T23:59:35","Observation","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","Stbd side light (primary) of Navigation light was out of order when inspected.","Navigation - Others","Navigation","Equipment Related","4.8","Medium","","","Fused light changed and confirmed operational. V-DJAG022785/19","2019-09-12T23:59:35","","Completed","2019-09-11T23:59:35","No","No","No","External"]
[null,null,null,274,null,"30_Mon Oct 07 2019 11:07:07 GMT+0000","2019-09-18T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Found one in No. Hydraulic Line of Remote Box (Port side Near Ballast tank Port #1 Leaking. ","Deck - Mooring Machinery","Mooring","Equipment Related","11.4","Very High","","","Due to Weather exposure condition of hose got detorated. Details sent to office and hose being procured to supply at next Port of call , singapore on 03rd Oct. 2019. Spares Received and changed the hydraulic Pipe. System tested. No leak. All satisfactory","2019-09-29T23:59:35","DJAG195050","Completed","2019-10-01T23:59:35","No","No","No","Internal"]
[null,null,null,275,null,"30_Mon Oct 07 2019 11:09:34 GMT+0000","2019-09-18T23:59:35","Defect","Ship Staff","Ship Staff Insp.","BWTS Autoback wsah filter Teflon Damaged, Require replacement. Electric Ballasting System Non Operational","Deck - Machinery","Cargo / Ballast Systems","Equipment Related","8.8","Medium","","","Teflon spacer replaced with new spacer.System is in operational condition now.                                V-DJAG024661/20","2020-03-24T23:59:35","DJAG190192","Completed","2020-02-21T23:59:35","No","No","No","Internal",""]
[null,null,null,374,null,"30_Mon Oct 07 2019 10:53:17 GMT+0000","2019-09-19T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Aft Stern Tube LO Pump Couplings worn out","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Require Replacement. Req Raised. Spares received and pump couplings alongwith Spider replaced. System tried out and put in use.","2019-09-23T23:59:35","DJAG190169","Completed","2019-09-21T23:59:35","No","No","No","Internal"]
[null,null,null,9362,null,"30_02/01/2020 1:39:37 PM","2019-09-20T23:59:35","Observation","Ship Staff","Ship Staff Insp.","During routine rounds on deck found half cut drums containing oil from manifold was left in the  midship store.","Miscellaneous","ISM Related","Human Error,Knowledge Based","5.11","Low","","","Immediately oil in the drum cleared. Drum cleaned dry.","2019-09-21T23:59:35","","Completed","2019-09-20T23:59:35","No","No","No","Internal"]
[null,null,null,6450,null,"30_Tue Jun 11 2019 22:11:52 GMT+0000 (Coordinated Universal Time)","2019-09-26T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Port LT Cooler Sea water Side Bottom Two in No's sacrificial Flanges leaking","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.3","Medium","","","Flanges replaced with new spare. Leaks eliminated V-DJAG023249/20","2019-10-30T23:59:35","","Completed","2019-10-29T23:59:35","No","No","No","Internal"]
[null,null,null,5697,null,"30_2019-11-03 12:46:05.000","2019-09-26T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Composite Boiler Feed water line leaking from gasket towards boiler side","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Boiler required to depressurize and rectify the leak. Compl;ete system isolated and rectified the leak. V-DJAG023282/20","2019-10-01T23:59:35","","Completed","2019-10-23T23:59:35","No","No","No","Internal"]
[null,null,null,7280,null,"30_Tue Oct 08 2019 18:04:47 GMT+0000 (Coordinated Universal Time)","2019-09-26T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Leak from AE FO Auto Filter seal. Filter required to be overhauled with New Seals.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.3","Medium","","","Required to Overhaul complete mechanism","2019-10-01T23:59:35","","Completed","2019-10-04T23:59:35","No","No","No","Internal"]
[null,null,null,9337,null,"30_Wed Jan 01 2020 06:33:17 GMT+0000","2019-09-26T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Rust stain appearing at the top of the lamp post and also all the flood lighting supports.","Elect. Mach. & Equip.","General Appearance","Equipment Related","11.11","Very High","","","De-rusted & re-painted. V-DJAG023319/20","2019-11-26T23:59:35","","Completed","2019-10-21T23:59:35","No","No","No","Internal"]
[null,null,null,9338,null,"30_Wed Jan 01 2020 06:41:01 GMT+0000","2019-09-26T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Bosun Store Supply Fan Vent Head is rusting.","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.12","Low","","","De-rust & re-painted. V-DJAG023320/20","2019-11-26T23:59:35","","Completed","2019-11-03T23:59:35","No","No","No","Internal"]
[null,null,null,9339,null,"30_Wed Jan 01 2020 06:43:38 GMT+0000","2019-09-26T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Bosun Store Supply Fan Starter weather protective box is not closing tight.","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.1","High","","","Renewed with a ready spare onboard. V-DJAG023321/20","2019-09-27T23:59:35","","Completed","2019-09-27T23:59:35","No","No","No","Internal"]
[null,null,null,9363,null,"30_02/01/2020 1:41:39 PM","2019-09-27T23:59:35","Observation","Ship Staff","Ship Staff Insp.","MAIN ENGINE HYDRAULIC PUMP CONNECTOR WORN OUT, PUMP IS ESSENTIAL FOR CARRYING OUT EMERGENCY MAINTENANCE ON MAIN ENGINE.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related,Human Error","10.32","Very High","","","IMMEDIATELY REPLACEMENT PUMP BROUGHT FROM SHORE FOR COMPLETING THE MAINTENANCE.","2019-09-27T23:59:35","","Completed","2019-09-27T23:59:35","No","No","No","Internal"]
[null,null,null,9364,null,"30_02/01/2020 1:43:43 PM","2019-10-11T23:59:35","Observation","Ship Staff","Ship Staff Insp.","During routine rounds in Engine room observed that the light inside the emergency escape at the bottom platform level was not operational.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related,External Factors","10.15","Low","","","The Light was immediately changed and confirmed operational.","2019-10-12T23:59:35","","Completed","2019-10-12T23:59:35","No","No","No","Internal"]
[null,null,null,5698,null,"30_2019-11-03 12:50:13.000","2019-10-21T23:59:35","Defect","Ship Staff","Ship Staff Insp.","AE #1 Unit 4 Fuel Pump got struck. up. Pump to overhaul and replace","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Pump replaced with new Pump V-DJAG023251/20","2019-10-21T23:59:35","","Completed","2019-10-21T23:59:35","No","No","No","Internal"]
[null,null,null,6448,null,"30_Tue Jun 11 2019 22:19:45 GMT+0000 (Coordinated Universal Time)","2019-10-25T23:59:35","Defect","Ship Staff","Ship Staff Insp.","SLOP PORT SAAB RADAR ULLAGE SYSTEM IN CCR SHOWN AS COMMUNICATION ERROR","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.12","Medium","","","INTERCHANGED CABLING TO ACCERTAIN ANETENA PROBLEM. NO PROBLEM WITH TANK UNIT AND CABLING FROM TANK TO CCR. REPLACED PCB IN CCR PANEL, PROBLEM DISAPPEARED FOR 10 HOURS AND AGAIN APPEARED. OFFICE INFORMED FOR EXPERTISE ADVICE V-DJAG023250/20","2020-01-23T23:59:35","DJAG190203","Completed","2019-11-08T23:59:35","No","No","No","Internal",""]
[null,null,null,7296,null,"30_Wed Dec 11 2019 13:47:48 GMT+0000 (Coordinated Universal Time)","2019-11-03T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Leak from M7 Mooring winch Speed adjusting lever Seal\t","Deck - Machinery","Mooring","Equipment Related","9.14","Medium","","","Removed top lever assembly and found O. Ring worn out. Replaced O. Ring with general O. Ring. System tried out, No leak from system V-DJAG023222/20","2019-12-04T23:59:35","","Completed","2019-12-04T23:59:35","No","No","No","Internal"]
[null,null,null,6449,null,"30_14/11/2019 7:27:01 AM","2019-11-06T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Gas Sampling Pump tripping","Cargo Mach.,Deck - Pipe / Fittings,Hull & Tanks","Cargo / Ballast Systems","Equipment Related","5.22","High","","","To overhaul pump. replace spares as required. Have spares onboard. Ship staff rectified on 16th NOV 2019 as per Chief Engineer's email to Kamal.","2019-11-09T23:59:35","","Completed","2019-11-09T23:59:35","No","No","No","Internal"]
[null,null,null,9365,null,"30_02/01/2020 1:46:13 PM","2019-11-08T23:59:35","Non Conformity","Ship Staff","Ship Staff Insp.","During routine rounds sighted the fire door leading from the staircase to the Sunken deck alleway was not closing properly.","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.35","Medium","","","1. The door closer for the Fire Door was immediately adjusted and the fire door checked and confirmed closing properly.","2019-11-08T23:59:35","","Completed","2019-11-08T23:59:35","No","No","No","Internal"]
[null,null,null,7048,null,"30_21/11/2019 3:49:23 PM","2019-11-09T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Boiler FO Supply PP #1 leaking from seal","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Boiler FO pump No 1 dismantled and overhauled with New Seal,Bearing and O rings. V-DJAG023469/20","2020-01-23T23:59:35","DJAG190199","Completed","2020-01-04T23:59:35","No","No","No","Internal",""]
[null,null,null,7052,null,"30_21/11/2019 3:41:32 PM","2019-11-09T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Noticed sacrificial Flange of No 2 main sea water pump in bad condition","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Removed Flange of Pump and found in bad condition, same replaced with onboard spare flange. V-DJAG023248/20","2019-11-10T23:59:35","","Completed","2019-11-10T23:59:35","No","No","No","Internal"]
[null,null,null,9366,null,"30_02/01/2020 1:47:59 PM","2019-11-09T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Found First aid and PPE box in BWTS room not secured properly and just left on deck.","Miscellaneous","ISM Related","Human Error,Knowledge Based","5.11","Low","","","Permanent Securing arrangement for Box made and put in place.","2019-11-13T23:59:35","","Completed","2019-11-14T23:59:35","No","No","No","Internal"]
[null,null,null,7051,null,"30_21/11/2019 3:25:06 PM","2019-11-11T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Stbd Windlass Hydraulic Brake Cylinder Leaking from Top Seal","Deck - Mooring Machinery","Mooring","Equipment Related","9.14","Medium","","","Seal to replace. Seal replaced with onboard spare seal. Also noted pitting on Hydraulic Shaft. Shaft to recondition in forth coming dry dock. Job added in REFMAN V-DJAG023311/20","2019-11-13T23:59:35","","Completed","2019-11-13T23:59:35","No","No","No","Internal"]
[null,null,null,7053,null,"30_21/11/2019 3:56:42 PM","2019-11-11T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Emergency Generator Exhausr Spark arrestor damaged. Accumlation of soot noticed at mouth of Exhaust outlet\t","Critical Equip.","Emgcy. Systems","Equipment Related","10.32","Very High","","","Replaced Spark arrestor mesh. cleaned the soot from mouth of exhaust","2019-11-14T23:59:35","","Completed","2019-11-14T23:59:35","No","No","No","Internal"]
[null,null,null,9336,null,"30_1/1/2020 6:31:54 AM","2019-11-12T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Solenoid Valve for Pumproom TRO unit is faulty.","Deck - Machinery","Cargo / Ballast Systems","Equipment Related","8.8","Medium","","","Solenoid valve replaced with new spare.                    V-DJAG024660/20","2020-03-24T23:59:35","DJAG190197","Completed","2020-02-21T23:59:35","No","No","No","Internal",""]
[null,null,null,7290,null,"30_Fri Dec 06 2019 11:04:19 GMT+0000 (Coordinated Universal Time)","2019-11-12T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Others (Eg. Insurance etc.)","12.20.05.011.04 Pre Arrival and Commencement Of Cargo Checklist - Sec. D Pt 4 Left Blank","Documentation","Cargo / Ballast Systems","Human Error","8.5","Very High","","","All deck Officers briefed and trained once again on the proper completion of checklists on the 29th Nov. 2019.  Deck officer on watch at the time of checklist completion to go through the checklists and ensure all points checked and no items missed out. Master to cross check before signing the checklist.","2019-12-03T23:59:35","","Completed","2019-11-22T23:59:35","No","No","No","Internal"]
[null,null,null,7291,null,"30_Fri Dec 06 2019 11:09:23 GMT+0000 (Coordinated Universal Time)","2019-11-12T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Others (Eg. Insurance etc.)","Hourly Loading Log for Cargo Loading Operation at FPSO N'Goma Angola on 07 ~ 08 Nov 2019 : Observed Non-nominated tanks 1C, 2P, 2S, 3C, 4P, 4S, 5C (Static Tanks) ullages remained constant to 2 decimal places for trim ranging from 0.0 to 4.3 Mtrs. \n\nUllages of Slop Tanks not recorded throughout the operation\n\n","Documentation","Cargo / Ballast Systems","Human Error","8.12","Medium","","","Training given to all deck officers on the 29th Nov. 2019. Importance of monitoring static tanks emphasised and explained to all once again. Deck officers instructed to closely monitor and record all tanks correct ullages after taking the readings from remote gauging system.","2019-12-03T23:59:35","","Completed","2019-11-22T23:59:35","No","No","No","Internal"]
[null,null,null,7292,null,"30_Fri Dec 06 2019 11:11:15 GMT+0000 (Coordinated Universal Time)","2019-11-12T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Others (Eg. Insurance etc.)","CCR Movement Log : Entry for Independent check of Line up did not include Venting during Loading at blue water sighted.","Documentation","Cargo / Ballast Systems","Human Error","8.5","Very High","","","Missed out entry discussed with all deck officers and training carried out once again. All deck officers instructed to ensure that the entry is not missed out in future.  Master to cross verify at the start of cargo operations. Training done on 29th Nov. 2019.","2019-12-03T23:59:35","","Completed","2019-11-22T23:59:35","No","No","No","Internal"]
[null,null,null,7293,null,"30_Fri Dec 06 2019 11:18:43 GMT+0000 (Coordinated Universal Time)","2019-11-12T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Bunkering Audit","Bunker Transfer Plan / Checklist 12.04.08.011.01 Section 7 - Monitoring of H2S/Benzene Vapors : \n\nBenzene reading measured by detector tubes shall be mentioned < Min value that can be measured by the specific tube. For example by Gastec tubes Min measurable value is 0.05 ppm, hence in that case benzene shall be mentioned <0.05 ppm (if no discoloration observed)\n\nUnderstand vessel has kept the Gas tubes as evidence of monitoring.\n\n","Documentation","Eng. / Strg. Comp.","Human Error,Knowledge Based","10.8","Medium","","","Noted, Have Benzene Test tube with least measurement of 0.1 PPM. As reading was less than 0.1 PPM in future will record the readings accordingly. All engineers have been trained and briefed regrading the same. Records will be cross checked by Chief eng. to ensure error is not repeated.","2019-12-03T23:59:35","","Completed","2019-11-20T23:59:35","No","No","No","Internal"]
[null,null,null,7294,null,"30_Fri Dec 06 2019 11:20:32 GMT+0000 (Coordinated Universal Time)","2019-11-12T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Bunkering Audit","Pt. 15 Bunker Safety Checklist dated 29 Oct 2019, it is mentioned Bunker tank contents to be monitored at intervals not exceeding 30 min. However no evidence of bunker soundings sighted between 2220 to 2315 Hrs on 29 Oct 2019 as per the Bunker Ullage sheet","Documentation","Eng. / Strg. Comp.","Human Error,Knowledge Based","10.8","Medium","","","Observation noted. All engineers briefed and trained to comply closely with the intervals as stated in the checklist. The ullage sheet and other docs to be cross checked by Chief engineer to avoid re-occurance.","2019-12-03T23:59:35","","Completed","2019-11-20T23:59:35","No","No","No","Internal"]
[null,null,null,7054,null,"30_30/11/2019 13:08:03","2019-11-19T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Deck seal Pump #1 Seal leaking","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Pump overhauled and replaced seal","2019-11-20T23:59:35","","Completed","2019-11-20T23:59:35","No","No","No","Internal"]
[null,null,null,7049,null,"30_30/11/2019 13:11:15","2019-11-21T23:59:35","Defect","Ship Staff","Ship Staff Insp.","BWTS Rectifier No 2 (Read as Rectifier B) tripping immediately after starting.","Deck - Machinery","Cargo / Ballast Systems","Equipment Related","8.8","Medium","","","Shunt for rectifier B isolated and opened up.Found one of the bi-polar plate defective.Same replaced with new spare.Now system in good order.                                                     V-DJAG024659/20","2020-03-24T23:59:35","DJAG190192","Completed","2020-02-11T23:59:35","No","No","No","Internal",""]
[null,null,null,7050,null,"30_Sun Dec 01 2019 07:29:58 GMT+0000 (Coordinated Universal Time)","2019-11-23T23:59:35","Defect","Ship Staff","Ship Staff Insp.","BWTS SYSTEM NON OPERATIONAL. TRC VALVE NOT RESPONDING","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.18","High","","","MESSAGE SENT TO OFFICE FOR MAKER'S ADVICE. FURTHER GOT ACCESS TO WINDOW SHOWING VALVE ISOLATED IN MANUAL MODE. RESET THE WINDOW TO AUTO MODE. SYSTEM OPERATIONAL. V-DJAG022873/19","2019-12-05T23:59:35","","Completed","2019-11-27T23:59:35","No","No","No","Internal",""]
[null,null,null,9272,null,"30_23/12/2019 3:39:11 PM","2019-12-02T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Aux engine t/charger turbine washing pressure reducing valve faulty.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Reducing valve replaced with spare received. V-DJAG023212/20","2020-03-02T23:59:35","DJAG190220","Completed","2019-12-21T23:59:35","No","No","No","Internal",""]
[null,null,null,7295,null,"30_Wed Dec 11 2019 03:22:13 GMT+0000 (Coordinated Universal Time)","2019-12-03T23:59:35","Defect","Ship Staff","Ship Staff Insp.","LEAK FROM SCRUBBER SEA WATER LINE NEAR SCRUBBER","Inert Gas","Cargo / Ballast Systems","Equipment Related","10.29","Medium","","","FOUND LEAK FROM FLANGE. REMOVED CONNECTION PIECE AND REPLACED GASKETS OF FLANGES. LEAK RECTIFIED V-DJAG023223/20","2019-12-04T23:59:35","","Completed","2019-12-04T23:59:35","No","No","No","Internal"]
[null,null,null,7297,null,"30_14/12/2019 5:35:51","2019-12-05T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Hydrophore Pump Motor tripping on start\t","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Checked, found contactor damaged. same replaced with equivalent ratings. System tried out, Performance satisfactory.V-DJAG023221/20","2019-12-05T23:59:35","","Completed","2019-12-05T23:59:35","No","No","No","Internal"]
[null,null,null,7298,null,"30_14/12/2019 5:39:36","2019-12-05T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Leakage from High pressure pipe line of Fuel oil AE #1 unit #4","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.19","Very High","","","Stopped generator. Replaced the leaking O. Rings. Leak rectified.V-DJAG023213/20","2019-12-05T23:59:35","","Completed","2019-12-05T23:59:35","No","No","No","Internal"]
[null,null,null,7299,null,"30_14/12/2019 14:48:34","2019-12-05T23:59:35","Defect","Ship Staff","Ship Staff Insp.","M/E Auto Back wash filter motor tripping\t","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Motor Jammed. opened up complete filter unit and overhauled. Cleared all obstruction and motor made operational V-DJAG023220/20","2019-12-05T23:59:35","","Completed","2019-12-05T23:59:35","No","No","No","Internal"]
[null,null,null,9274,null,"30_23/12/2019 12:17:07 PM","2019-12-06T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Slop tank STBD level gauging TGU defective.","Elect. Mach. & Equip.","Cargo / Ballast Systems","Equipment Related","8.19","High","","","TGU replaced with new spare and system is operational now. V-DJAG023318/20","2020-01-28T23:59:35","","Completed","2019-12-14T23:59:35","No","No","No","Internal"]
[null,null,null,9367,null,"30_02/01/2020 1:49:53 PM","2019-12-08T23:59:35","Non Conformity","Ship Staff","Ship Staff Insp.","During routine rounds it was noticed that the Steering gear checklist displayed in the Steering gear room was not updated for the last Steering Gear test .","Documentation","Eng. / Strg. Comp.","Human Error","10.39","High","","","1. The checklist was immediately updated with the latest information and date.","2019-12-09T23:59:35","","Completed","2019-12-09T23:59:35","No","No","No","Internal"]
[null,null,null,9273,null,"30_23/12/2019 3:43:55 PM","2019-12-14T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Main engine unit no 1 cylinder oil injection pressure found less as compared to other units.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Lubricator renewed with the new spare.                 V-DJAG024658/20","2020-03-14T23:59:35","","Completed","2019-12-19T23:59:35","No","No","No","Internal"]
[null,null,null,9725,null,"30_12/1/2020 9:19:50 AM","2019-12-25T23:59:35","Defect","Ship Staff","Ship Staff Insp.","INERT GAS SYSTEM PLC ABNORMAL CPU AND I/O FAIL ALARM","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.25","Very High","","","PLC FAIL CARD (PF-024) RELAY (RX) FOUND DEFECTIVE, SAME REPLACED AND SYSTEM BECAME NORMAL.                                                V-DJAG023262/20","2020-03-25T23:59:35","","Completed","2019-12-26T23:59:35","No","No","No","Internal"]
[null,null,null,10545,null,"30_27/1/2020 1:25:18 PM","2020-01-14T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Unit No 1 fuel oil high pressure pipe from fuel actuator to ditributor block leaking.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","High pressure pipe removed and O rings renewed. V-DJAG023880/20","2020-04-14T23:59:35","","Completed","2020-01-16T23:59:35","No","No","No","Internal"]
[null,null,null,10546,null,"30_27/1/2020 1:28:03 PM","2020-01-14T23:59:35","Defect","Ship Staff","Ship Staff Insp.","AFT mooring winches remote operation lever block leaking of lube oil.","Deck - Mooring Machinery","Mooring","Equipment Related","4.3","Medium","","","Hydraulic lever block isolated and O ring renewed. V-DJAG023896/20","2020-04-14T23:59:35","","Completed","2020-01-16T23:59:35","No","No","No","Internal"]
[null,null,null,10544,null,"30_29/1/2020 1:58:10 PM","2020-01-21T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Leak observed from the main Engine Unit no 1 HCU block.Found One of the allen plug of the HCU has developed crack.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Plug replaced with new one after receiving spares. V-DJAG024993/20","2020-04-21T23:59:35","DJAG200011","Completed","2020-03-19T23:59:35","No","No","No","Internal",""]
[null,null,null,10753,null,"30_16/2/2020 11:22:34 AM","2020-01-30T23:59:35","Defect","Ship Staff","Ship Staff Insp.","MAIN ENGINE JACKET COOLING WATER CONTROLLER MALFUNCTIONING.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.38","Medium","","","JACKET WATER CONTROLLER AUTO CALLIBRATION AND ZERO CALLIBRATION CARRIED OUT. CONTROLLER TRIED OUT AND NOW WORKING SATISFACTORY.                              V-DJAG024657/20","2020-04-29T23:59:35","","Completed","2020-02-04T23:59:35","No","No","No","Internal"]
[null,null,null,10754,null,"30_7/3/2020 9:20:57 AM","2020-02-09T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Both Anchor windlass hydraulic brake\n\nspring tension marking on spindle is not matching with the set mark.","Deck - Mooring Machinery","Mooring","Equipment Related","9.2","Very High","","","Both widlass brake adjustment carried out.                V-DJA024630/20","2020-05-13T23:59:35","","Completed","2020-02-13T23:59:35","No","No","No","Internal"]
[null,null,null,10755,null,"30_7/3/2020 9:41:23 AM","2020-02-19T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Vibration observed from the HFO purifier No 1 motor side.","E/R - Purifier","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Purifier stopped and inspected. Found Friction pads securing bolts sheared off and coupling bearing damaged. Same renewed and purifier started.Running satisfactory.                                   V-DJAG024631/2","2020-05-19T23:59:35","","Completed","2020-02-21T23:59:35","No","No","No","Internal"]
[null,null,null,11650,null,"30_03/05/2020 22:36:39","2020-03-02T23:59:35","Observation","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","A few computers were missing USB Locks","Miscellaneous","General Appearance","Equipment Related","7.15","High","","","Requested Office/Management for USB Locks and rcvd confirmation on 23 Mar 2020 about being delivered to vessel. Vessel received on the 16-06-2020 @Singapore.","2020-06-23T23:59:35","USB locks are non PO item. Capt Jupji will supply to vessel separately.","Completed","2020-06-10T23:59:35","No","No","No","External",""]
[null,null,null,11651,null,"30_03/05/2020 22:46:40","2020-03-02T23:59:35","Observation","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","SCBA Air Bottle connection was found leaking.","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.43","High","","","Rectified immediatley","2020-06-02T23:59:35","","Completed","2020-03-02T23:59:35","No","No","No","External"]
[null,null,null,10767,null,"30_12/3/2020 8:11:00 AM","2020-03-03T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Deck seal pump no 2 seal leaking.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Deck seal pump no 2 leaking from the mechanical seal.\n\nPump opened up, parts cleaned and inspected. Found Mechanical seal damaged and impeller shaft have pitting marks all over the place where the stationery part of the seal sits.\n\nRequisition raised for the new parts.\n\nPump boxed back with new seal and o ring. Pump started and running satisfactorily without any leaks. V-DJAG016364/18","2020-06-04T23:59:35","","Completed","2020-03-04T23:59:35","No","No","No","Internal"]
[null,null,null,11174,null,"30_5/4/2020 12:29:15 PM","2020-03-14T23:59:35","Defect","Ship Staff","Ship Staff Insp.","BWTS PORT SIDE FILTER AUTO BACKFLUSH MOTOR TRIPPING ON OVERLOAD","Deck - Machinery","Cargo / Ballast Systems","Equipment Related","8.8","Medium","","","Port side filter isolated and opened up.All filter candles removed and filter housing lifted up.Found teflon spacer in good condition and motor is getting overloaded because of backflushing rotating arm touching the bottom of the candles bottom plate.Both the surfaces cleaned and filter assembled.Port filter tried out and now in operational condition.                                  V-DJAG025614/20","2020-06-14T23:59:35","","Completed","2020-04-23T23:59:35","No","No","No","Internal",""]
[null,null,null,11175,null,"30_22/3/2020 8:26:53 AM","2020-03-14T23:59:35","Defect","Ship Staff","Ship Staff Insp.","MAIN AIR COMPRESSOR NO 2 NON RETURN VALVE IN THE FINAL AIR DELIVERY LINE LEAKING.","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","NON RETURN VALVE RENEWED.                                V-DJAG024850/20","2020-06-14T23:59:35","","Completed","2020-03-14T23:59:35","No","No","No","Internal"]
[null,null,null,11652,null,"30_03/05/2020 22:50:32","2020-03-18T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Wash basin in duty mess was found leaking.","Accommodation","General Appearance","Human Error","11.13","Low","","","Wash Basin in the Duty mess was found leaking water from the lip of the Wash basin sitting/resting on the wooden Table. This wash Basin was never being used for any washing purposes, however was put in use by Shore Personnel @ Singapore when the Leak was observed. See LPSQ (DJAG/INA/2020/01).","2020-06-18T23:59:35","","Completed","2020-03-29T23:59:35","No","No","No","Internal"]
[null,null,null,11653,null,"30_03/05/2020 23:07:10","2020-03-18T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","No gangway placard or briefing carried out.","Documentation","ISM Related","Knowledge Based","5.15","Medium","","","Vessel was still in the process of Anchoring, with Bridge watch Level – 4, No Ships Personnel available at Gangway when Visitors boarded the Vessel. Off watch personnel to be present at the Gangway to receive visitors. See LPSQ (DJAG/INA/2020/01).","2020-06-13T23:59:35","","Completed","2020-04-15T23:59:35","No","No","No","Internal"]
[null,null,null,11654,null,"30_03/05/2020 23:12:44","2020-03-18T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Ship shore safety check list for last discharge operations point # 29 “The agreed tank venting system will be used” answered as NO VENTING VESSEL DISCHARGING","Documentation","ISM Related","Knowledge Based","5.9","Very High","","","Vessel was Discharging, therefore during Key Meeting with Loading Master, Chief Officer mentioned point # 29 as “NO VENTING, VESSEL DISCHARGING, whereas “NO VENTING, IGS IN USE” shall be mentioned in the future. See LPSQ (DJAG/INA/2020/01).","2020-06-13T23:59:35","","Completed","2020-04-18T23:59:35","No","No","No","Internal"]
[null,null,null,11655,null,"30_03/05/2020 23:17:00","2020-03-18T23:59:35","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","PPE poster used onboard is an old version","Accommodation","ISM Related","Knowledge Based","5.5","Low","","","There was a ambiguity as to which Matrix was the latest version as a few of them posted on Bulkheads had version – 03. All crew members & Officers must have kept a track of it. This was brought to attention of Auditor who then confirmed that 12.06.15.001.01 is the latest version. Latest version posters replaced. See LPSQ (DJAG/INA/2020/01).","2020-06-13T23:59:35","","Completed","2020-04-08T23:59:35","No","No","No","Internal"]
[null,null,null,11656,null,"30_03/05/2020 23:22:19","2020-03-18T23:59:35","Non Conformity","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Garbage kept outside ECR in a plastic bag and same was not segregated.","Miscellaneous","General Appearance","Human Error","10.29","Medium","","","Wiper was told to empty garbage bins from the ECR.After collecting the garbage,he kept it outside of ECR instead of garbage locker as was assigned another job.Same was corrected when noticed during the internal audit. See LPSQ (DJAG/INA/2020/01).","2020-06-13T23:59:35","","Completed","2020-03-18T23:59:35","No","No","No","Internal"]
[null,null,null,11658,null,"30_03/05/2020 23:01:35","2020-03-18T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Accommodation doors were closed and locked from inside using special locking arrangement.","Accommodation","ISPS Related","Inappropriate Procedure","7.12","High","","","Vessel was still in the process of Anchoring, with Bridge watch Level – 4, All Ships Personnel were engaged in Vsl Arrival at Singapore and anchoring. This job was supposed to be done after vessel anchored, which was missed out as all personnel got busy even before vessel anchored. See LPSQ (DJAG/INA/2020/01)","2020-06-18T23:59:35","","Completed","2020-04-15T23:59:35","No","No","No","Internal"]
[null,null,null,11439,null,"30_Thu Apr 16 2020 07:05:16 GMT+0000","2020-03-18T23:59:35","Defect","Ship Staff","Ship Staff Insp.","3 GALLEY BAKING OVENS  - LOW INSULATION DUE TO HEATING ELEMENTS DEFECTIVE.","Accommodation","General Appearance","Equipment Related","11.16","Low","","","REQUISITION RAISED FOR SPARE PARTS.Both Heating element replaced with new spare, Insulation megger tested found readings more than 1000 Mega Ohms, System powered up found working in good order.Un planned Job order No. V-DJAG026825/20","2020-06-26T23:59:35","DJAG200098","Completed","2020-06-30T23:59:35","No","No","No","Internal",""]
[null,null,null,11176,null,"30_5/4/2020 12:07:34 PM","2020-03-23T23:59:35","Defect","Ship Staff","Ship Staff Insp.","ME LO PURIFIER BELT BROKEN","E/R - Purifier","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","ME LO purifier driving belt found broken.\n\nPurifier bowl dismantled and 4000 hrs routine carried out.\n\nVertical shaft removed and new belt installed.Purifier boxed back with new O rings.\n\nPurifier started and running satisfactorily.                  V-DJAG017864/19","2020-06-23T23:59:35","","Completed","2020-03-25T23:59:35","No","No","No","Internal"]
[null,null,null,11440,null,"30_Thu Apr 16 2020 07:08:51 GMT+0000","2020-03-27T23:59:35","Defect","Ship Staff","Ship Staff Insp.","GALLEY ICE CUBE MACHINE NON OPERATION DUE TO WATER PUMP DEFECTIVE.","Accommodation","General Appearance","Equipment Related","11.16","Low","","","REQUISITION RAISED FOR SPARE PARTS..---- SPARES RECIEVD AT SINGAPORE ON 16.06.2020 AND REPLACED THE SAME AND SYSTEM WORKING SATISFACTORY.                                           V-DJAG026486/20","2020-06-26T23:59:35","DJAG200099","Completed","2020-06-10T23:59:35","No","No","No","Internal",""]
[null,null,null,11441,null,"30_Thu Apr 16 2020 07:11:29 GMT+0000","2020-03-27T23:59:35","Defect","Ship Staff","Ship Staff Insp.","GALLEY - BRAISING PAN GIVES LOW INSULATION DUE TO DEFECTIVE HEATING ELEMENT.","Accommodation","General Appearance","Equipment Related","11.16","Low","","","SPARE PARTS REQUISITION RAISED.Vessel recieved new spares at Singapore, same replaced and system tested working in order. UPJR- V-DJAG026736/20","2020-06-26T23:59:35","DJAG200100","Completed","2020-06-16T23:59:35","No","No","No","Internal",""]
[null,null,null,11657,null,"30_03/05/2020 22:42:43","2020-03-28T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Speed Log sensor showing erratic reading.","Navigation - Echo Sounder / Speed Log","Navigation","Equipment Related","4.14","Very High","","","Transducer got shifted/lifted up due to Slamming/pitching of the vessel. Entry made into the forepeak tank and Transducer removed, cleaned and fitted back after the height adjustment as per manual.Now in operational condition. V-DJAG025540/20","2020-06-27T23:59:35","","Completed","2020-04-09T23:59:35","No","No","No","Internal"]
[null,null,null,11436,null,"30_Thu Apr 16 2020 06:54:13 GMT+0000","2020-04-02T23:59:35","Defect","Ship Staff","Ship Staff Insp.","GREY WATER OVERBOARD LINE PIPE SECTION  IS LEAKING.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","SECTION OF THE PIPE REMOVED AND LEAKAGE ARRESTED BY WELDING IN E/R WORKSHOP. PIPE FITTED BACK AND PUT IN USE.NO LEAKAGE OBSERVED. WILL BE RAISING REQUISITION FOR THE SAME SIZE PIPE SO THAT CAN BE REPLACED NEXT TIME.V-DJAG025263/20","2020-07-03T23:59:35","","Completed","2020-04-03T23:59:35","No","No","No","Internal"]
[null,null,null,11816,null,"30_13/5/2020 2:17:39 PM","2020-04-28T23:59:35","Defect","Ship Staff","Ship Staff Insp.","ECR unit cooler No 2 not operational.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","New Compressor Type : One-stage hermetic scroll . Model : ZB38KQE,. Manufacturer : EMERSON . Cooling capacity : 17.4 kW (15,000 kcal/h) at Te=+ 5.0? and Tc=+ 45.0? recieved at Singapore on 16.06.2020, Same fitted in place, Vaccumn the system and Charged gas. System put in service . Working in order. Unplanned Maintance Job Order - VDJAG026760/20","2020-07-29T23:59:35","DJAG 200117","Completed","2020-06-27T23:59:35","No","No","No","Internal",""]
[null,null,null,11818,null,"30_07/05/2020 22:53:42","2020-04-29T23:59:35","Defect","Ship Staff","Ship Staff Insp.","CO2 bottles securing clamps inspected and found 25 Pieces Having cracks.","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.4","High","","","25 pieces of securing clamps renewed with spare clamps,monitoring the remaining in place securing clamps.JOB No.V-DJAG026912/20","2020-06-23T23:59:35","","Completed","2020-07-04T23:59:35","No","No","No","Internal",""]
[null,null,null,11817,null,"30_13/5/2020 2:07:40 PM","2020-05-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Aft mooring winches starter panel PLC not working after siwtched on/off for the maintenance.","Deck - Mooring Machinery","Mooring","Equipment Related","9.14","Medium","","","No Spare PLC onboard. Office has been informed and awaiting maker's advice. Emergency operating procedure received and tested. Working satisfactory. VESSEL RECIEVED NEW PLC AT FUJAIRAH, OLD DEFECTIVE PLC REPLACED WITH NEW AS PER MAKER PROCEDURE / INSTRUCTIONS. SYSTEM TRIED OUT WORKING  IN ORDER. UNPLANNED JOB ORDER NO: V-DJAG026824/20","2020-07-24T23:59:35","DJAG200182","Completed","2020-06-30T23:59:35","No","No","No","Internal",""]
[null,null,null,11819,null,"30_13/05/2020 3:00:21","2020-05-03T23:59:35","Defect","Ship Staff","Ship Staff Insp.","SOME OF THE BUNKER VALVES ARE HARD AND DIFFICULT TO OPERATE.","Deck - Pipe / Fittings","General Appearance","Equipment Related","6.7","High","","","ALL FO BUNKER VALVES WORM GEAR ACTUATOR ASSEMBLY DISMANTLED.OLD GREASE REMOVED AND GEARS CLEANED.FRESH GREASE APPLIED AND NOW IN GOOD WORKING ORDER.                     V-DJAG025874/20","2020-08-03T23:59:35","","Completed","2020-05-05T23:59:35","No","No","No","Internal"]
[null,null,null,11820,null,"30_14/05/2020 0:33:20","2020-05-05T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Composite boiler bracing/top supporting arrangement nuts found to be slack/loosed.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","All Nuts tightened.                                                 V-DJAG025939/20","2020-08-05T23:59:35","","Completed","2020-05-06T23:59:35","No","No","No","Internal"]
[null,null,null,11967,null,"30_01/06/2020 11:16:15","2020-05-05T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Bunkering Audit","Repetitive checks were not carried out as per bunker (VLSFO) safety checklist \n\nIt states repetitive checks to be carried every 0.5 hour, However checks were carried out at 1 hour interval.\n\n","Documentation","Eng. / Strg. Comp.","Inappropriate Procedure","","","","","Discussed in tool box meeting. Checks were made frequently, but recorded as one hour as enough space was not available in check list and bunker duration was long. Advised to maintain repetitive checks duration not more than one hour.","2020-08-05T23:59:35","","Completed","2020-05-20T23:59:35","No","No","No","Internal"]
[null,null,null,11969,null,"30_01/06/2020 11:19:48","2020-05-05T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Cargo Audit","12.04.08.014.00 Code \"A\" to be signed by both parties.","Documentation","Cargo / Ballast Systems","Inappropriate Procedure","","","","","12.04.08.014.00 Code \"A\" signed by both parties","2020-08-05T23:59:35","","Completed","2020-05-20T23:59:35","No","No","No","Internal"]
[null,null,null,11821,null,"30_13/5/2020 1:56:53 PM","2020-05-06T23:59:35","Defect","Ship Staff","Ship Staff Insp.","During routine rounds of the engine room , found Anti Splash tape is missing for few Main Engine high pressure pipes.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.19","Very High","","","Anti splash tape applied to all the high pressure pipes where it was missing.                                         V-DJAG025887/20","2020-08-06T23:59:35","","Completed","2020-05-06T23:59:35","No","No","No","Internal"]
[null,null,null,11968,null,"30_01/06/2020 11:22:30","2020-05-15T23:59:35","Defect","Ship Staff","Ship Staff Insp.","MAIN ENGINE LO COOLER 3-WAY VALVE CONTROLLER MALFUNCTIONING AND RESPONDING ERRATICALLY.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.38","Medium","","","AUTO CALLIBRATION OF THE CONTROLLER DONE AND NOW WORKING SATISFACTORY.               V-DJAG026146/20","2020-08-15T23:59:35","","Completed","2020-05-19T23:59:35","No","No","No","Internal"]
[null,null,null,12802,null,"30_08/06/2020 19:10:54","2020-05-27T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Forward Electric whistle non- Operational.","Navigation - Others","Navigation","Equipment Related","4.7","High","","","Forward Electric Whistle removed from the location and dismantlled. Found driven gear damaged. Cannibilized spares from the former whistle and is working good now. However, requisition raised for the newer spares.","2020-10-24T23:59:35","DJAG200189 and DJAG205075","Completed","2020-10-24T23:59:35","No","No","No","Internal",""]
[null,null,null,12803,null,"30_08/06/2020 18:48:39","2020-05-31T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Emergency fire pump leaking from the mechanical seal","LSA / FFA","Eng. / Strg. Comp.","Equipment Related","5.41","Very High","","","Pump dismantled and overhauled with new mechanical seal.                                                                O-DJAG001133/16                                                                   ","2020-08-31T23:59:35","","Completed","2020-06-02T23:59:35","No","No","No","Internal"]
[null,null,null,12804,null,"30_08/06/2020 19:04:52","2020-05-31T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Main air compressor cooler gasket leaking.","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Air Compressor isolated and depressurised.Cooler removed and gasket renewed. V-DJAG026369/20.","2020-08-31T23:59:35","","Completed","2020-05-31T23:59:35","No","No","No","Internal"]
[null,null,null,13179,null,"30_17/07/2020 19:28:27","2020-06-10T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Control Cable for E/R Crane damaged.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","8.5","Very High","","","Control Cable renewed with spare received.Job Order No.-V-DJAG027110/20","2020-09-08T23:59:35","","Completed","2020-07-23T23:59:35","No","No","No","Internal",""]
[null,null,null,13282,null,"30_1/8/2020 5:51:59 PM","2020-06-29T23:59:35","Defect","Ship Staff","Ship Staff Insp.","ME UNIT # 5 CYL COVER JW OUTLET TEMP GIVING ERRATIC READING","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","8.13","Medium","","","Cylinder Cover Jacket Water Outlet Sensor renewed with new spare received onboard.Job Order No-V-DJAG028010/20","2020-09-29T23:59:35","DJAG200219","Completed","2020-09-01T23:59:35","No","No","No","Internal",""]
[null,null,null,13289,null,"30_30/7/2020 6:01:37 PM","2020-07-03T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Exhaust Gas Economizer Exh Gas  Manometer found empty and non functional.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Manometer connections opened up once Engine stopeed,lines cleared,water added with distinguishable coulour and made operational.JOB ORDER NO.V-DJAG027111/20","2020-08-13T23:59:35","","Completed","2020-07-15T23:59:35","No","No","No","Internal"]
[null,null,null,13283,null,"30_31/07/2020 12:00:39 AM","2020-07-09T23:59:35","Defect","Ship Staff","Ship Staff Insp.","PORT / STBD HOSE HANDLING CRANE OPEARTING LEVER'S WERE NOT FREE TO OPERATE","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.5","Very High","","","VESSEL OVERHAULED STBD SIDE CONTROL BLOCK ON 27 AUG 2020.OVERHAULED PORT SIDE CONTROL BLOCK ON 07 SEP 2020.","2020-09-03T23:59:35","","Completed","2020-08-31T23:59:35","No","No","No","Internal",""]
[null,null,null,13284,null,"30_31/07/2020 12:04:57 AM","2020-07-10T23:59:35","Defect","Ship Staff","Ship Staff Insp.","DURING ROUTINE INSPECTION IT WAS OBSERVED THAT 1P SBT VENT HEAD FLOAT WAS CRACKED AND FILLED WITH WATER","Hull & Tanks","Cargo / Ballast Systems","Equipment Related","11.7","High","","","RENEWED WITH SPARE FLOAT ONBOARD","2020-10-24T23:59:35","DJAG200212","Completed","2020-11-01T23:59:35","No","No","No","Internal",""]
[null,null,null,13285,null,"30_31/07/2020 12:09:12 AM","2020-07-10T23:59:35","Observation","Ship Staff","Mooring Audit","ROPE TAILS EXCEEDED MORE THAN 18 MONTHS IN SERVICE","Deck - Mooring Machinery","Mooring","Equipment Related","9.17","High","","","VESSEL RECEIVED 20 PCS NEW ROPE TAILS IN SINGAPORE ON 18 NOV 20.","2020-10-24T23:59:35","DJAG205009","Completed","2020-11-11T23:59:35","No","No","No","Internal",""]
[null,null,null,13286,null,"30_31/07/2020 12:14:24 AM","2020-07-10T23:59:35","Defect","Ship Staff","Ship Staff Insp.","LIFEBOAT EXTERNAL LIGHT EXPIRED AND NOT HAVING SUFFICIENT ILLUMINATION, INDENSITY OF LIGHT IS  NOT UPTO THE STANDARDS","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.29","High","","","VESSEL RECEIVED NEW EXTERNAL LIGHT AND SAME HAS BEEN REPLACED.OPERATION TESTED, ALL FOUND IN ORDER","2020-09-08T23:59:35","DJAG200213","Completed","2020-08-29T23:59:35","No","No","No","Internal",""]
[null,null,null,16930,null,"30_Sun Jan 10 2021 23:56:58 GMT+0000","2020-07-20T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Main Deck No.5 Flood Light Lamp Post rusting.","Elect. Mach. & Equip.","General Appearance","Equipment Related","11.11","Very High","","","De-rusted & newly painted.","2020-10-19T23:59:35","","Completed","2020-10-21T23:59:35","No","No","No","Internal"]
[null,null,null,16931,null,"30_Mon Jan 11 2021 00:08:44 GMT+0000","2020-07-20T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Bosun Store Supply Fan vent head rusting.","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.12","Low","","","De-rusted & newly painted during DD.","2020-10-19T23:59:35","","Completed","2020-11-01T23:59:35","No","No","No","Internal"]
[null,null,null,16932,null,"30_Mon Jan 11 2021 00:25:42 GMT+0000","2020-07-20T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Bosun Store Supply Fan Starter weather protective box is not closing tight.","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.10","Medium","","","Renewed with a  ROB spare.","2020-10-19T23:59:35","","Completed","2020-09-27T23:59:35","No","No","No","Internal"]
[null,null,null,16933,null,"30_Mon Jan 11 2021 00:29:14 GMT+0000","2020-07-20T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Port LT Cooler SW side, bottom two pcs sacrificial flanges leaking.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Renewed with spare during DD.","2020-10-19T23:59:35","","Completed","2020-11-01T23:59:35","No","No","No","Internal"]
[null,null,null,16934,null,"30_Mon Jan 11 2021 00:32:26 GMT+0000","2020-07-20T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Aux Eng FO Auto Filter leaking.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Renewed with one ROB spare seal.","2020-10-19T23:59:35","","Completed","2020-10-04T23:59:35","No","No","No","Internal"]
[null,null,null,16935,null,"30_Mon Jan 11 2021 00:34:56 GMT+0000","2020-07-20T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Composite Boiler feedwater line leaking towards the Boiler side.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Renewed the flange gasket.","2020-08-03T23:59:35","","Completed","2020-07-25T23:59:35","No","No","No","Internal"]
[null,null,null,13467,null,"30_15/08/2020 1:18:25","2020-08-02T23:59:35","Defect","Ship Staff","Ship Staff Insp.","SERVICE AIR COMPRESSOR PRESSURE SWITCH MALFUNCTIONING.","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Pressure Switch Renewed and Found Satisfactory","2020-10-24T23:59:35","DJAG200225","Completed","2020-10-23T23:59:35","No","No","No","Internal",""]
[null,null,null,13468,null,"30_15/08/2020 1:21:57","2020-08-05T23:59:35","Defect","Ship Staff","Ship Staff Insp.","NO.2 MAIN AIR COMPRESSOR INTERCOOLER GASKET LEAK.","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Intercooler Gasket Renewed with Original Maker's Spare received onboard.Job Order No.-V-DJAG028012/20","2020-10-05T23:59:35","DJAG200105","Completed","2020-08-27T23:59:35","No","No","No","Internal",""]
[null,null,null,13466,null,"30_15/08/2020 1:41:19","2020-08-06T23:59:35","Defect","Ship Staff","Ship Staff Insp.","No.1 MAIN AIR COMPRESSOR AIR OUTLET NON RETURN VALVE OBSERVED LEAKING.","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Non Return Valve replaced with new spare received onboard.Job Order No.-V-DJAG028011/20","2020-10-06T23:59:35","DJAG200106","Completed","2020-08-27T23:59:35","No","No","No","Internal",""]
[null,null,null,13470,null,"30_15/08/2020 1:01:04 PM","2020-08-06T23:59:35","Defect","Ship Staff","Ship Staff Insp.","During routine inspection it was observed that STBD side manifold spill oil tank drain line plug was missing  which is non compliance of VIQ 7 , 6.8  which states that Drain and vents should be fitted with valves and either capped or plugged .This is to inform you that  vessel does not having spare drain plug for the same.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","6.8","High","","","VESSEL PLACED A NEW DRAIN PLUG ","2020-09-23T23:59:35","","Completed","2020-08-27T23:59:35","No","No","No","Internal",""]
[null,null,null,13471,null,"30_15/08/2020 1:04:13 PM","2020-08-06T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Vessel carried out Slop tanks steam coil pressure testing and observed leakage from return line drain valves. Vessel tried to overhaul the valves but whilst opening the valve all the bolts were getting broken and overhauled only one valve but that too not holding.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.15","High","","","RENEWED WITH SPARE VALVES RECEIVED IN SINGAPORE ON 18 NOV 20.","2020-10-24T23:59:35","DJAG205085","Completed","2020-11-20T23:59:35","No","No","No","Internal",""]
[null,null,null,13899,null,"30_01/09/2020 16:26:38","2020-08-19T23:59:35","Defect","Ship Staff","Ship Staff Insp.","No.2 HFO PURIFIER PT5-WATER PRESSURE SENSOR MALFUNCTIONING.","E/R - Purifier","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Received the New Sensor and assembled,found satisfactory","2020-11-19T23:59:35","DJAG200232","Completed","2020-11-15T23:59:35","No","No","No","Internal",""]
[null,null,null,13900,null,"30_01/09/2020 16:31:56","2020-08-20T23:59:35","Defect","Ship Staff","Ship Staff Insp.","During alarms testing,Incinerator low negative combustion pressure switch observed not operating and alarm not activating.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Switch replaced with new spare.Unplanned Job Order No. V-DJAG029410/20","2020-10-20T23:59:35","DJAG200233","Completed","2020-11-09T23:59:35","No","No","No","Internal",""]
[null,null,null,13986,null,"30_09/09/2020 12:41:16 AM","2020-09-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","NO.1 ECDIS (STBD SIDE) LCD Monitor cooling fan & Central control unit (CCU) fan has passed the exchange recommended  time.","Navigation - ECDIS","Navigation","Equipment Related","4.7","High","","","Cooling fan renewed","2020-10-23T23:59:35","DJAG200235","Completed","2020-11-21T23:59:35","No","No","No","Internal",""]
[null,null,null,13987,null,"30_08/09/2020 2:09:05 PM","2020-09-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","vessel has carried out routine overhauling of vent riser breather valve ( Valve no . IG54) & below condition observed :1.Damaged diaphragm.Vessel does not having the spare for the same.\n\n\n\n2.Observed moderate pitting all around the disc .Tried out lapping but no improvement.3.Observed severe pitting and worn out seat .","Inert Gas","Cargo / Ballast Systems","Equipment Related","8.19","High","","","Mast riser breather valve replaced with new valve received in Onsan, Korea","2021-01-24T23:59:35","DJAG200234","Completed","2021-01-11T23:59:35","No","No","No","Internal",""]
[null,null,null,13988,null,"30_08/09/2020 2:22:06 PM","2020-09-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Observed minor leakage from No.2 electric driven ballalst pump upper seal","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.8","Medium","","","NO.2 electric ballast pump overhauled in drydock","2020-10-23T23:59:35","","Completed","2020-11-01T23:59:35","No","No","No","Internal",""]
[null,null,null,13989,null,"30_15/9/2020 3:41:05 PM","2020-09-03T23:59:35","Defect","Ship Staff","Ship Staff Insp.","No.1 AC Compressor Motor Failure during operation.Windings found burnt.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Motor renewed with new spare.Unplanned Job Order No.-V-DJAG029411/20","2020-11-23T23:59:35","DJAG205089","Completed","2020-11-12T23:59:35","No","No","No","Internal",""]
[null,null,null,13990,null,"30_15/9/2020 4:08:38 PM","2020-09-04T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Two exhaust bellows(EXP-6 and EXP-7) in the Main Engine Exhaust Line found with cracks during inspection.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Bellows replaced with new spare.Unplanned job order no.V-DJAG029412/20","2020-11-23T23:59:35","DJAG205083","Completed","2020-10-26T23:59:35","No","No","No","Internal",""]
[null,null,null,13993,null,"30_15/9/2020 3:46:26 PM","2020-09-05T23:59:35","Defect","Ship Staff","Ship Staff Insp.","MAIN LO COOLER 3 WAY TEMPERATURE CONTROLLER POSITIONER VALVE FOUND BEHAVING ERRATICALLY.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","AUTO CALIBRATION OF THE POSITIONER CONTROLLER CARRIED FAILED.POSITIONER CONTROOLER REPLACED WITH NEW SPARE AND TRIED OUT.JOB ORDER N0-V-DJAG028053/20.","2020-09-23T23:59:35","","Completed","2020-09-05T23:59:35","No","No","No","Internal"]
[null,null,null,13991,null,"30_15/9/2020 3:59:40 PM","2020-09-07T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Main Engine No.2 Turbocharger outlet Bellow found cracked during inspection.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Bellows replaced with new spare.Unplanned job order no.V-DJAG029412/20","2020-11-23T23:59:35","DJAG205090","Completed","2020-10-26T23:59:35","No","No","No","Internal",""]
[null,null,null,13992,null,"30_16/9/2020 3:52:31 PM","2020-09-08T23:59:35","Defect","Ship Staff","Ship Staff Insp.","While overhauling No.1 SG Oil Air cooler fan motor,motor cooling fan found in disintergrated condition.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Boxed back No.1 SG Oil Air cooler fan motor and put in use without the motor cooling fan.Portable Cooling Fan Received and Installed,Found Satisfactory","2020-11-23T23:59:35","DJAG200237","Completed","2020-11-15T23:59:35","No","No","No","Internal",""]
[null,null,null,14179,null,"30_28/9/2020 3:43:42 PM","2020-09-09T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Excessive vibration and noise on filter backflushing system for BWTS experienced on sister vessels with similar systems due to excessive backflushing water.","Cargo Mach.,Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","6.21","High","","","Orifice plates inserted on the discharge side of backflush pump for both the BWTS filtes in pumproom.","2020-11-23T23:59:35","Maker auto supply. No need PO number.","Completed","2020-11-25T23:59:35","No","No","No","Internal",""]
[null,null,null,14180,null,"30_30/9/2020 1:51:39 PM","2020-09-11T23:59:35","Defect","Ship Staff","Ship Staff Insp.","FRESH WATER TANK (S) OUTLET VALVE OBSERVED LEAKING.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Valve Renewed with spare.JO Number V-DJAG029415/20","2020-11-23T23:59:35","","Completed","2020-10-28T23:59:35","No","No","No","Internal",""]
[null,null,null,14181,null,"30_23/09/2020 2:38:50 PM","2020-09-13T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Please note that vessel carried out pre-arrival preparation to dockyard for changing wires for Gangway, Lifeboats , Hose handling carne ,Provision crane and Rescue davits  and Observed deep groove over on arc for the distance of approximately 3 cm on stbd side Accommodation ladder guide sheave and Over on arc for the distance of approximately 2.5 cm on Port side shifting guide roller.","Deck - Machinery","Structural Condn. / WT integrity ","Equipment Related","5.47","Medium","","","Renewed with spare sheaves onboard.","2020-10-23T23:59:35","DJAG200238","Completed","2020-11-20T23:59:35","No","No","No","Internal",""]
[null,null,null,14182,null,"30_23/09/2020 2:42:16 PM","2020-09-13T23:59:35","Defect","Ship Staff","Ship Staff Insp.","During routine checks , it was observed that stbd side bridge door packing was damaged. Light test carried out and test fail","Accommodation","General Appearance","Equipment Related","11.6","Medium","","","Packing renewed with spare packing received from drydock.","2020-10-23T23:59:35","DJAG200240","Completed","2020-11-18T23:59:35","No","No","No","Internal",""]
[null,null,null,14183,null,"30_25/09/2020 4:23:38 AM","2020-09-13T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Some of the light's switch in crews cabin in accomodation is working in erratic manner and requires couple times on / off  when it actually lights up.","Accommodation","MLC Related","Equipment Related","11.16","Low","","","Switches are being changed with available spare onboard. New switches will be ordered in the forthcoming electrical store requisition and replacement of remaining switches will be carried out.","2020-10-23T23:59:35","","Completed","2020-11-15T23:59:35","No","No","No","Internal",""]
[null,null,null,14184,null,"30_30/9/2020 9:33:48 AM","2020-09-17T23:59:35","Defect","Ship Staff","Ship Staff Insp.","While overhauling No.3 ME Hyd Top Bracing,it was observed that the check valve between primary and secondary chamber for was completely shattered and inoperational.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Spares Received and waiting for anchoarge period to remove complete top bracing unit.","2021-01-24T23:59:35","DJAG200247","Completed","2021-01-18T23:59:35","No","No","No","Internal",""]
[null,null,null,14185,null,"30_30/9/2020 9:38:00 AM","2020-09-17T23:59:35","Defect","Ship Staff","Ship Staff Insp.","While overhauling No.2 ME Hyd Top Bracing,it was observed that the cyl cover was cracked and the ram had excessive pitting.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Renewed the cylinder covered and seal,found satisfactory","2021-01-24T23:59:35","DJAG200247","Completed","2021-01-15T23:59:35","No","No","No","Internal",""]
[null,null,null,14186,null,"30_01/10/2020 11:28:21 AM","2020-09-23T23:59:35","Defect","Ship Staff","Ship Staff Insp.","The Navtex printout quality from navtex receiver printer is not consistent. Sometimes printout is not legible . It can be vetting and PSC observations.","Navigation - GMDSS & Communication","Navigation","Equipment Related","4.7","High","","","Navtex printer renewed.","2020-11-08T23:59:35","DJAG200250","Completed","2020-11-20T23:59:35","No","No","No","Internal",""]
[null,null,null,14187,null,"30_01/10/2020 12:24:43 PM","2020-09-23T23:59:35","Defect","Ship Staff","Ship Staff Insp.","During routine inspection it was observed that most of the mooring winches gear oil level glas faded and unable to read .","Deck - Mooring Machinery","Mooring","Equipment Related","9.14","Medium","","","All mooring winch sight glass renewed.","2020-11-23T23:59:35","DJAG200248","Completed","2020-11-20T23:59:35","No","No","No","Internal",""]
[null,null,null,14188,null,"30_01/10/2020 12:41:41 PM","2020-09-23T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Vessel observed leakage from control block operating lever of mooring winches WMW1,WMW2,M1,M4,M6 due to damged o-ring/ Shaft seal / Step seals","Deck - Mooring Machinery","Mooring","Equipment Related","9.14","Medium","","","Vessel has rectified all leaking operating levers of mooring winches. Vessel raised requisition DJAG200248 for spare of o-ring, shaft seal and step seals for remaining winches.","2020-11-23T23:59:35","DJAG200248","Completed","2020-11-05T23:59:35","No","No","No","Internal",""]
[null,null,null,15286,null,"30_16/10/2020 2:17:32 PM","2020-10-05T23:59:35","Defect","Ship Staff","Ship Staff Insp.","MAIN ENGINE JACKET COOLING WATER CONTROLLER MALFUNCTIONING.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.38","Medium","","","Controller renewed with spare.JO No.V-DJAG029416/20","2020-12-19T23:59:35","DJAG205081","Completed","2020-11-12T23:59:35","No","No","No","Internal"]
[null,null,null,15287,null,"30_16/10/2020 2:22:13 PM","2020-10-05T23:59:35","Defect","Ship Staff","Ship Staff Insp.","ME UNIT # 5 CYL COVER JW OUTLET TEMP GIVING ERRATIC READING","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","8.32","Low","","","Swnsor renewed with spare.Job Order No.-V-DJAG029417/20","2020-12-23T23:59:35","DJAG200257","Completed","2020-10-29T23:59:35","No","No","No","Internal"]
[null,null,null,15288,null,"30_19/10/2020 2:00:48 PM","2020-10-07T23:59:35","Defect","Ship Staff","Ship Staff Insp.","During cargo operations,noticed that the fore peak tank level gauge transmitter showing erratic readings.\t","Hull & Tanks","Cargo / Ballast Systems","Equipment Related","11.7","High","","","Fore peak Tank Level Gauge Transmitter to be renewed.Requisition number DJAG200259 raised. Level gauge transmitter renewed in drydock.","2020-10-23T23:59:35","DJAG200259","Completed","2020-10-28T23:59:35","No","No","No","Internal"]
[null,null,null,15453,null,"30_04/12/2020 2:02:44 PM","2020-11-11T23:59:35","Observation","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","Cargo system sea valves testing arrangement did not provide a pressure regulator to  avoid surge pressure exceeding in the system more than 3.5 kglcm2 during testing.","Miscellaneous","Cargo / Ballast Systems","Equipment Related","6.4","High","","","Pressure regulator arrangement prepared and installed.","2020-11-13T23:59:35","","Completed","2020-11-13T23:59:35","No","No","No","External"]
[null,null,null,15284,null,"30_20/11/2020 1:21:54 PM","2020-11-11T23:59:35","Defect","Ship Staff","Ship Staff Insp.","ME Lo backwash By-pass filter outlet butterfly valve leaking.LO leaking from the valve stem packing.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Gland Packing Added and Found Satisfactory","2020-12-11T23:59:35","","Completed","2020-11-19T23:59:35","No","No","No","Internal",""]
[null,null,null,17613,null,"30_25/01/2021 1:41:36 AM","2020-11-11T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Cargo Audit","Cargo: Recording/Monitoring of cargo seachest pressure was not consistent in hourly log  during discharging operation(Zhoushan, China-Nov 2020)","Miscellaneous","Cert. & Docu.","Human Error","8.5","Very High","","","All duty officers were briefed about the consequences of not monitoring/ recording cargo seachest pressure. Chief officer/Duty officer to cross audit the forms/ logs intermitteltly during operations closely and ensure all OOW are filling up their respective logs properly.","2021-02-10T23:59:35","","Completed","2021-01-10T23:59:35","No","No","No","Internal"]
[null,null,null,17614,null,"30_25/01/2021 1:44:46 AM","2020-11-11T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Cargo Audit","Cargo: Old discharge plan/forms were in use for discharge operation at Zhoushan, China-Nov 2020","Miscellaneous","Cert. & Docu.","Human Error","8.5","Very High","","","All officers/ trainees were briefed about the short coming and a short training session was carried out on how to print latest forms/ checklists/permits directly from QDMS.                                                           Also in addition the importance of using latest forms/ checklist/permits was highlighted and the consequences of not using as well.","2021-02-10T23:59:35","","Completed","2021-01-10T23:59:35","No","No","No","Internal"]
[null,null,null,15285,null,"30_20/11/2020 1:51:02 PM","2020-11-12T23:59:35","Defect","Ship Staff","Ship Staff Insp.","ER crane traverse movement motor winding burn.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.28","Low","","","Motor renewed  and tried out the crane,foun satisfactory","2020-12-23T23:59:35","DJAG200279","Completed","2020-12-22T23:59:35","No","No","No","Internal",""]
[null,null,null,16389,null,"30_23/12/2020 3:49:27 AM","2020-11-18T23:59:35","Non Conformity","Ship Staff","Ship Staff Insp.","ISPS visitor card no.14 misplaced. Unable to locate the card.","Miscellaneous","ISPS Related","Human Error,Inappropriate Procedure","7.12","High","","","-Thorugh search and investigation carried out for missing ISPS visitor card..\n\n-Crew/Officer briefing w.r.t monitoring of ISPS visitor cards.\n\n","2021-01-18T23:59:35","","Completed","2020-11-21T23:59:35","No","No","No","Internal"]
[null,null,null,15452,null,"30_04/12/2020 14:01:01","2020-11-24T23:59:35","Defect","Ship Staff","Ship Staff Insp.","GMDSS Battery out of 4,1 PCS of battery is Defective.","Navigation - GMDSS & Communication","Safety / LSA / FFA","Equipment Related,External Factors","4.7","High","","","Renewed with spare new one ,found satisfactory","2021-01-24T23:59:35","","Completed","2021-01-15T23:59:35","No","No","No","Internal",""]
[null,null,null,15624,null,"30_15/12/2020 14:08:41","2020-12-03T23:59:35","Defect","Ship Staff","Ship Staff Insp.","LO Purifier during desludge interval giving discharge feedback \" P161\"  error alarm once in every five or six discharge interval.","E/R - Purifier","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","As per makers troubleshooting carried out,found satisfactory","2020-12-23T23:59:35","","Completed","2020-12-20T23:59:35","No","No","No","Internal"]
[null,null,null,18200,null,"30_04/03/2021 18:12:51","2020-12-25T23:59:35","Defect","Ship Staff","Ship Staff Insp.","AUS VACUUM PUMP #2 Grease cup glass found in broken condition.","Cargo Mach.,Deck - Machinery","Cargo / Ballast Systems","Equipment Related,External Factors,Inappropriate Procedure","8.8","Medium","","","Renewed with the new spare, which received from Linggi, Malaysia on 01-July-2021","2021-07-08T23:59:35","DJAG210015","Completed","2021-06-24T23:59:35","No","No","No","Internal",""]
[null,null,null,17549,null,"30_15/1/2021 10:48:14 AM","2020-12-26T23:59:35","Defect","Ship Staff","Ship Staff Insp.","OWS Electric Heater giving low insulation alarm","Critical Equip.","MARPOL Related","Equipment Related,External Factors","6.14","High","","","Checked and found one coil is in damaged condition,need to be renewed heater","2021-03-23T23:59:35","DJAG210020","Completed","2021-02-24T23:59:35","No","No","No","Internal",""]
[null,null,null,17550,null,"30_06/01/2021 4:16:58 PM","2020-12-29T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Port Provision Crane Emergency Operation Quick Coupler connection are slightly leaking for Hydraulic Oil.","Deck - Machinery","Eng. / Strg. Comp.","Equipment Related,External Factors","8.5","Very High","","","Temporarily NRV Ball valve are blanked and  Press fit,covered with Denso tape.Need to be renewed.","2021-03-23T23:59:35","DJAG210028","Completed","2021-02-25T23:59:35","No","No","No","Internal",""]
[null,null,null,17551,null,"30_15/01/2021 8:05:23 PM","2020-12-29T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Foam Pump line (BF-50 SDNR & BF-51 Flushing valve) found leaking.","LSA / FFA","Safety / LSA / FFA","Behaviour Based,Equipment Related,Human Error,Inappropriate Procedure","5.39","Very High","","","New valves received at Singapore on 19 Jan 2021 and renewed.","2021-01-24T23:59:35","DJAG210001","Completed","2021-01-14T23:59:35","No","No","No","Internal",""]
[null,null,null,18023,null,"30_28/02/2021 6:58:36 AM","2021-01-06T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Anemometer Cup out of 3,1 pcs in damaged condition","Elect. Mach. & Equip.,Navigation - Others","Navigation","Equipment Related,External Factors,Inappropriate Procedure","4.7","High","","","Cup is renewed.","2021-03-23T23:59:35","DJAG210042","Completed","2021-03-02T23:59:35","No","No","No","Internal",""]
[null,null,null,17609,null,"30_29/01/2021 10:16:25 AM","2021-01-10T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Em.Generator Switchboard 440V Earth Fault meter intermittenly malfunctioning.","Critical Equip.,Elect. Mach. & Equip.","Emgcy. Systems","Equipment Related","10.32","Very High","","","Meter to be renewed.","2021-03-23T23:59:35","DJAG210046","Completed","2021-02-24T23:59:35","No","No","No","Internal",""]
[null,null,null,17610,null,"30_22/01/2021 11:57:45 AM","2021-01-12T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ANCHOR hawse pipe cover to be cropped in order to secure properly.","Miscellaneous","ISPS Related","Equipment Related","9.18","Low","","","Hawse pipe cropped to fit in place","2021-02-12T23:59:35","","Completed","2021-02-05T23:59:35","No","No","No","Internal",""]
[null,null,null,17611,null,"30_22/01/2021 12:00:18 PM","2021-01-12T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Mooring winch linkages to be de-rusted","Deck - Mooring Machinery","General Appearance","Equipment Related","9.18","Low","","","Completed derusting & painting of mooring winch linkages completed, same reported in weekly report","2021-08-24T23:59:35","","Completed","2021-08-18T23:59:35","No","No","No","Internal",""]
[null,null,null,17612,null,"30_22/01/2021 12:03:42 PM","2021-01-12T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Ramp on main deck to be de-rusted.","Miscellaneous","General Appearance","Equipment Related","11.3","Medium","","","De rusting of main deck ramps completed","2021-03-24T23:59:35","","Completed","2021-03-13T23:59:35","No","No","No","Internal",""]
[null,null,null,17615,null,"30_22/01/2021 16:14:06","2021-01-12T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ME Manoeuvring platform tube light not working need to be replaced","Elect. Mach. & Equip.","General Appearance","Equipment Related,External Factors,Human Error,Inappropriate Procedure","10.15","Low","","","Tube light renewed.","2021-02-11T23:59:35","","Completed","2021-01-13T23:59:35","No","No","No","Internal"]
[null,null,null,17616,null,"30_22/01/2021 16:07:28","2021-01-12T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","There is one very big wooden box which is not labelled as to what spare is inside.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related,Inappropriate Procedure","10.29","Medium","","","box opened and all spare inside secured.","2021-02-11T23:59:35","","Completed","2021-01-17T23:59:35","No","No","No","Internal"]
[null,null,null,17617,null,"30_22/01/2021 16:15:31","2021-01-12T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ME FO Supply pump grounding wire damaged","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related,External Factors,Human Error,Inappropriate Procedure","10.23","Medium","","","wire installed and connected.","2021-02-11T23:59:35","","Completed","2021-01-22T23:59:35","No","No","No","Internal"]
[null,null,null,17618,null,"30_22/01/2021 16:03:48","2021-01-12T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Sea water line flange passing in the way of HFO transfer pump starter panel to be covered by tape","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.23","Medium","","","flange covered with tapre and insulated","2021-02-11T23:59:35","","Completed","2021-01-23T23:59:35","No","No","No","Internal"]
[null,null,null,17619,null,"30_22/01/2021 16:18:46","2021-01-12T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","#4 E/R Fan fire damper cannot fully close when activated","LSA / FFA","ISM Related","Equipment Related,External Factors,Human Error,Inappropriate Procedure","10.18","High","","","Checked and adjusted ram for closing,tried out damper closing fully.","2021-01-18T23:59:35","","Completed","2021-01-16T23:59:35","No","No","No","Internal"]
[null,null,null,17620,null,"30_22/01/2021 16:09:25","2021-01-12T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ME LO Backwash filter slight leak from top cover need to be rectified","E/R - Main Engine","General Appearance","Equipment Related,Human Error,Inappropriate Procedure","10.32","Very High","","","filter changeover to by pass filter,top cover o-ring renewed.tried out found no leak.","2021-02-11T23:59:35","","Completed","2021-01-21T23:59:35","No","No","No","Internal"]
[null,null,null,17621,null,"30_22/01/2021 16:12:23","2021-01-12T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","BLR Chemical dosing pump save all tray need to be chipped and paint.","Miscellaneous","General Appearance","Equipment Related,Human Error,Inappropriate Procedure","10.29","Medium","","","cleaned,painted","2021-02-11T23:59:35","","Completed","2021-01-18T23:59:35","No","No","No","Internal"]
[null,null,null,17622,null,"30_22/01/2021 16:10:56","2021-01-12T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Old damaged Spare Forward Whistle motor not secured in spare room","Miscellaneous","Eng. / Strg. Comp.","Equipment Related,Human Error,Inappropriate Procedure","10.29","Medium","","","secured with proper securing arrangement,same labeled","2021-02-11T23:59:35","","Completed","2021-01-21T23:59:35","No","No","No","Internal"]
[null,null,null,18024,null,"30_19/02/2021 3:09:25","2021-02-11T23:59:35","Defect","Ship Staff","Ship Staff Insp.","AE#2 Lub Oil Cooler Outlet shut off cock are leaking from body.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related,External Factors,Human Error","10.32","Very High","","","Temporarily o-ring has added in gland working satisfactory.Spare already placed on board .","2021-07-24T23:59:35","DJAG210035","Completed","2021-02-12T23:59:35","No","No","No","Internal",""]
[null,null,null,18025,null,"30_25/02/2021 5:04:28 PM","2021-02-14T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Electric Ballast pump Filter Unit HMI Display is continuously flickering and intermittently frozen","Cargo Mach.,Deck - Machinery,Elect. Mach. & Equip.","Cargo / Ballast Systems","Equipment Related,External Factors,Inappropriate Procedure","6.21","High","","","Rnewed with new spare.","2021-07-08T23:59:35","DJAG210058","Completed","2021-06-25T23:59:35","No","No","No","Internal",""]
[null,null,null,18022,null,"30_26/02/2021 8:33:18 PM","2021-02-17T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Vessel short of low expansion foam by approx. 200 litres in foam tank(Fixed fire fighting system for deck)","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.4","High","","","260 ltrs of foam received at Singapore on 02 Mar 2021. Foam tank topped up to require level.","2021-05-17T23:59:35","DJAG210036","Completed","2021-02-24T23:59:35","No","No","No","Internal",""]
[null,null,null,18026,null,"30_25/02/2021 18:33:23","2021-02-17T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Meat Room evaporator drain try heater cable malfunctioning.","Elect. Mach. & Equip.","MLC Related","Equipment Related,External Factors,Inappropriate Procedure","10.32","Very High","","","Replaced old heater with new spare heater. Tried out, found working satisfactory.","2021-07-24T23:59:35","DJAG210062","Completed","2021-07-19T23:59:35","No","No","No","Internal",""]
[null,null,null,18027,null,"30_26/02/2021 8:40:12 PM","2021-02-17T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Securing brackets/supports of main deck ramps corroded/ wasted in few locations.","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","Equipment Related","11.5","Medium","","","Temporary cold work repair carried out. Hot work to be carried out in dry dock for permanent repairs.Transferred to Ref Man","2023-05-23T23:59:35","","Completed","2021-03-08T23:59:35","Yes","No","No","Internal",""]
[null,null,null,25949,null,"30_Sat Jul 02 2022 04:00:56 GMT+0000","2021-02-21T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Aft Peak Tank outlet FCV unit Actuator cylinder in corroded and damaged state,unable to carried out auto operation for the valve","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","6.21","High","","","Received the valve and kept as Spare , presently valve is functioning satisfactory after overhaul.","2022-06-23T23:59:35","DJAG210144","Completed","2022-06-23T23:59:35","No","No","No","Internal"]
[null,null,null,18202,null,"30_06/03/2021 17:28:03","2021-02-24T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Stern Tube Air Seal unit  Glass is on crack condition.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related,External Factors,Human Error,Inappropriate Procedure","10.32","Very High","","","Temporarily repaired carried out. Working satisfactorily. Also New spare placed on board.","2021-07-08T23:59:35","DJAG210070","Completed","2021-06-25T23:59:35","No","No","No","Internal",""]
[null,null,null,18203,null,"30_06/03/2021 17:33:02","2021-02-26T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Officer Recreation Room Fan motor in burn condition.(Inslutaion Low \"0\")","Accommodation,Elect. Mach. & Equip.","MLC Related","Equipment Related,External Factors,Inappropriate Procedure","10.32","Very High","","","Fitted new duct fan in Officer's Recreation Room. Tried out found working satisfactory.","2021-07-24T23:59:35","DJAG210075","Completed","2021-07-19T23:59:35","No","No","No","Internal",""]
[null,null,null,18199,null,"30_08/03/2021 4:47:19 PM","2021-03-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","AUXILIARY ENGINE #1 ROU UNIT PCB FAILURE","E/R - Aux. Engine,Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related,External Factors,Inappropriate Procedure","10.32","Very High","","","Temporarily repaired working satisfactory.Spare already placed on board .","2021-07-24T23:59:35","DJAG210078","Completed","2021-03-01T23:59:35","No","No","No","Internal",""]
[null,null,null,18204,null,"30_15/03/2021 18:40:13","2021-03-08T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Main Air Compressor#1 Rubber Coupling found in damaged condition","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related,External Factors,Inappropriate Procedure","10.32","Very High","","","Renewed the coupling","2021-03-24T23:59:35","DJAG210011","Completed","2021-03-20T23:59:35","No","No","No","Internal",""]
[null,null,null,18605,null,"30_10/04/2021 12:45:04 PM","2021-03-24T23:59:35","Observation","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","4.25 : The vessels \"TRON 40VDR\" float free EPIRB VDR capsule was not tested monthly per the manufacturers recommendations. Discussions with vessel personnel revealed that while the Normal test was being conducted, the recommended monthly Extended test, (testing that includes the EPIRBs GPS function) had not been conducted for at least four months. (There were no records found indicating that the extended test had been conducted.)\n\n","Navigation - GMDSS & Communication","Communication","Equipment Related","4.25","Low","","","Extended test for VDR EPIRB carried out.","2021-04-23T23:59:35","","Completed","2021-03-25T23:59:35","No","No","No","External"]
[null,null,null,18606,null,"30_10/04/2021 1:06:46 PM","2021-03-24T23:59:35","Observation","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","The mooring tails were constructed of polyamide but there was no evidence that the stated LDBF of tails was 125% of mooring wire MBL when wet. The certificates did not specify \"Break tested wet\" as recommended(MEG4 5.2.1 under Line Design Breaking Force). It was also noted that the tails in use had a diameter 84 mm and a stated LDBF of 159.6 mt . There were also two spare polyamide tails though , that had a diameter of 96mm and a LDBF of 158.6 mt , further suggesting that the tails in use were possibly undersized. Certificates for both types of tails indicated that the certificates were as per MEG4.","Miscellaneous","Mooring","Equipment Related","9.5","High","","","Following explanation from manufacturer :                           1. The tails had been tested in WET conditions, you can find attached the revised Certificates mentioning specially that. However this is a specific term of MEG4 and if someone wants to mention compliance to MEG4 then for sure all tails (specially Nylon which have significant difference) should be tested always under wet conditions.  I will inform my secretary to update all of your certs for DHT Jaguar.\n\n2. We will do for all tails and will revert\n\n3. We face this difference with almost all NYLON tails of competitors specially when competitors are from Asia area origin. This huge difference comes firstly from the High Quality of raw material that we use for Nylon. This material comes 100% from European origin and cannot be compared to the quality used from many competitors. We had placed from the past goals with high performance for our Nylon raw material. It is all about the Tenacity of the raw material yarn and if recycled or not. Of course the braiding lay and structure is also a second factor but it is not easy to explain over email. In this point I will take the opportunity to inform you and your offices if   superintendents , captains, technicians etc of your company I  could arrange a web meeting with our Technical support team & me to solve any query you may have and discuss in details the Nylon tails details etc. At your interest you can give me the emails of your colleagues interested and my specialist will create a hostage link for the meeting over (Teams, Webex or any platform you use)\n\n4. The figure NSBF is the relevant \"Actual Breaking\" that we were talking on MEG3 and the LDBF is like the \" Minimun Breaking Load\"\n\n","2021-04-23T23:59:35","","Completed","2021-03-29T23:59:35","No","No","No","External"]
[null,null,null,18604,null,"30_08/04/2021 12:47:08 PM","2021-03-30T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Main deck walkways found lacking anti-skid in many locations.","Miscellaneous","General Appearance","External Factors","11.3","Medium","","","Walkways de rusted and painted with anti skid.","2021-05-23T23:59:35","","Completed","2021-05-13T23:59:35","No","No","No","Internal",""]
[null,null,null,18607,null,"30_13/04/2021 22:02:19","2021-03-30T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Boiler heater steam inlet valve leaking","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Gasket renewed , leakage rectified.","2021-04-03T23:59:35","","Completed","2021-03-30T23:59:35","No","No","No","Internal"]
[null,null,null,18608,null,"30_15/04/2021 16:17:03","2021-03-30T23:59:35","Defect","Ship Staff","Ship Staff Insp.","AE 3 NO. 1  UNIT TEMPRATURE SENSOR DAMAGE","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","AE 3 UNIT NO.1 TEMPRATURE SENSOR RENEWED WITH SPARE ONE","2021-03-30T23:59:35","","Completed","2021-03-30T23:59:35","No","No","No","Internal"]
[null,null,null,18609,null,"30_13/04/2021 22:10:30","2021-03-31T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Jacket cooling water preheater steam inlet valve leaking","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Gasket renewed , leakage rectified .","2021-04-03T23:59:35","","Completed","2021-03-31T23:59:35","No","No","No","Internal"]
[null,null,null,18610,null,"30_13/04/2021 22:13:45","2021-03-31T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Fresh water generator feed line leakage","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Pipe removed gasket renewed, leakage rectified.","2021-04-03T23:59:35","","Completed","2021-03-31T23:59:35","No","No","No","Internal"]
[null,null,null,18611,null,"30_15/04/2021 16:24:58","2021-04-03T23:59:35","Defect","Ship Staff","Ship Staff Insp.","AUX. BOILER CHEMICAL DOSING PUMP SEAL LEAKING","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","AUX. BOILER CHEMICAL DOSING PUMP SEAL RENEWED","2021-04-05T23:59:35","","Completed","2021-04-03T23:59:35","No","No","No","Internal"]
[null,null,null,18612,null,"30_15/04/2021 16:30:22","2021-04-06T23:59:35","Defect","Ship Staff","Ship Staff Insp.","NO.2 REFER COMPRESSOR MECHANICAL SEAL LEAKING","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","MECHANICAL SEAL RENEWED , LEAKAGE RECTIFIED.","2021-04-06T23:59:35","","Completed","2021-04-06T23:59:35","No","No","No","Internal"]
[null,null,null,18603,null,"30_15/04/2021 16:21:13","2021-04-08T23:59:35","Defect","Ship Staff","Ship Staff Insp.","AUX SEA WATER PUMP MECHANICAL SEAL LEAKING","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","MECHANICAL SEAL RENEWED.","2021-06-23T23:59:35","","Completed","2021-04-16T23:59:35","No","No","No","Internal",""]
[null,null,null,19068,null,"30_27/4/2021 9:00:34 PM","2021-04-19T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Steering gear weather tight door gasket found leaky, cause ingress of water in steering gear room.","Miscellaneous","Structural Condn. / WT integrity ","Equipment Related","11.6","Medium","","","packing checked, found in good condition. Door locking system tightened and found in good condition.","2021-05-18T23:59:35","","Completed","2021-04-20T23:59:35","No","No","No","Internal"]
[null,null,null,19521,null,"30_16/05/2021 7:32:53","2021-04-26T23:59:35","Defect","Ship Staff","Ship Staff Insp.","KONGSBERG SYSTEM DISPLAYING WRONG DATE AND TIME ON BRIDGE TELEGRAPH AND ER AMS PANELS.","Miscellaneous,Navigation - Others","Navigation","Equipment Related","10.32","Very High","","","FOLLOWING MAKER'S ADVISE, SUCESSFULLY CHANGED DATE FROM BIOS SETTINGS.","2021-07-25T23:59:35","","Completed","2021-05-29T23:59:35","No","No","No","Internal",""]
[null,null,null,19523,null,"30_10/5/2021 8:14:52 PM","2021-04-30T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Leakage in sea water inlet line of forward hydraulic oil cooler","Deck - Machinery","Mooring","Equipment Related","9.18","Low","","","Leakage rectified by fabricating new section of pipe line.","2021-05-07T23:59:35","","Completed","2021-05-01T23:59:35","No","No","No","Internal"]
[null,null,null,19522,null,"30_10/5/2021 8:22:42 PM","2021-05-03T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Compressor of No.1 ECR Unit Cooler is non operational and showing zero insulation.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Replaced with ne compressor, now both ECR Unit Coolers are working satisfactory.","2021-07-23T23:59:35","DJAG210096","Completed","2021-07-20T23:59:35","No","No","No","Internal",""]
[null,null,null,19524,null,"30_12/5/2021 7:28:00 PM","2021-05-04T23:59:35","Defect","Ship Staff","Ship Staff Insp.","AE 2 UNIT NO. 5 EXHAUST GAS TEMPRETURE SENSOR DEFECTIVE ","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","DEFECTIVE SENSOR RENEWED , FAULT RECTIFIED .","2021-05-05T23:59:35","","Completed","2021-05-04T23:59:35","No","No","No","Internal"]
[null,null,null,19525,null,"30_15/05/2021 7:18:40","2021-05-07T23:59:35","Defect","Ship Staff","Ship Staff Insp.","GUIDE STOPPER FOR MAIN STARTING AIR VALVE SHEARED.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","STOPPER PLATE REMOVED FROM PLACE. NEW GUIDE STOPPER FABRICATED AND INSTALLED. PLATE PUT BACK IN PLACE.\n\nVALVE TRIED OUT. ALL SATISFACTORY.","2021-05-08T23:59:35","","Completed","2021-05-07T23:59:35","No","No","No","Internal"]
[null,null,null,19611,null,"30_28/05/2021 12:00:10","2021-05-12T23:59:35","Defect","Ship Staff","Ship Staff Insp.","EXHAUST PIPE FOR EMERGENCY DG, FOUND WASTED/CORRODED AND REPAIRED WITH CORDOBOND.","Critical Equip.","Emgcy. Systems","Equipment Related","10.32","Very High","","","PIPE REMOVED FROM PLACE AND BROUGHT TO ER WORKSHOP. CROPPED , NEW PIPE FABRICATED AND PUT BACK IN PLACE.","2021-05-23T23:59:35","","Completed","2021-05-13T23:59:35","No","No","No","Internal"]
[null,null,null,19681,null,"30_03/06/2021 7:44:53 PM","2021-05-27T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Portside hose handling crane level gauge leaking from the bottom part.","Deck - Machinery","Cargo / Ballast Systems","Equipment Related","8.5","Very High","","","Received & replaced with spares  level gauge receivd at Singapore on 12 Dec 2021","2021-12-24T23:59:35","DJAG210116","Completed","2021-12-09T23:59:35","No","No","No","Internal",""]
[null,null,null,19682,null,"30_04/06/2021 7:16:13","2021-05-27T23:59:35","Defect","Ship Staff","Ship Staff Insp.","BOTH FW TANK LEVEL GUAGES ARE IRRACTIC AND DOESN'T SHOW THE TRUE LEVEL OF THE TANK","Hull & Tanks","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","BOTH LEVEL GUAGE RENEWED AND CALIBRATED..JOB REPORTED AS UNPLANNED IN PAL.JOB REF NO-V-DJAG037429/21.","2021-12-08T23:59:35","DJAG210118","Completed","2021-12-08T23:59:35","No","No","No","Internal",""]
[null,null,null,19684,null,"30_05/06/2021 5:57:49","2021-05-28T23:59:35","Defect","Ship Staff","Ship Staff Insp.","COMPOSITE BOILER FEED PUMP NO.2 LEAKY MECHANICAL SEAL.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","SEAL RENEWED WITH SPARE. PUMP PUT BACK IN USE.","2021-06-03T23:59:35","","Completed","2021-05-28T23:59:35","No","No","No","Internal"]
[null,null,null,19683,null,"30_11/6/2021 4:12:49 PM","2021-06-03T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Sewage treatment plant, discharge pump cut out level sensor was malfunctioning due to water ingress inside same opened and repaired and sealed back using silicone. Same repairs carried out on high level alarm sensor as well as it was erratic. Also the timer of sewage blower is non-operational the blower keeps on running continuously.","Elect. Mach. & Equip.","MARPOL Related","Equipment Related","10.32","Very High","","","New level switches and timer installed System operational.unplanned job no-V-DJAG037487/21 reported in pal.","2021-12-24T23:59:35","","Completed","2021-12-10T23:59:35","No","No","No","Internal",""]
[null,null,null,20200,null,"30_26/07/2021 8:16:41 PM","2021-06-25T23:59:35","Observation","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","The magnetic compass located on the monkey island was noted with an approx. 3 cm diameter bubble along with few tiny bubbles on the compass bowl","Navigation - Others","Navigation","Equipment Related","4.9","Medium","","","Rectified prior to the close out meeting.","2021-07-03T23:59:35","","Completed","2021-06-25T23:59:35","No","No","No","External"]
[null,null,null,20201,null,"30_26/07/2021 8:22:09 PM","2021-06-25T23:59:35","Observation","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","It was not evident that a Cold Work Permit was used for the main engine scavenge space cleaning and inspection carried out on 6 May 2021 as verified with the Chief Engineer onboard. Only the enclosed space checklist, man hole opening permit and\n\nisolation permit was noted in use. The risk assessment carried out for the said job required the cold work permit to be used as per the risk identified.","Documentation","Safety / LSA / FFA","Inappropriate Procedure,Knowledge Based","5.2","Very High","","","On departure from port of inspection, the vessel’s superintendent discussed the observation and guidance from the company procedures on permit to work systems with\n\nthe senior management. After the briefing, a training session for the crew was carried out on\n\nthe company’s permit to work system and risk assessment process for a strict future\n\ncompliance with the requirements laid down by the company.","2021-07-03T23:59:35","","Completed","2021-06-28T23:59:35","No","No","No","External"]
[null,null,null,20085,null,"30_12/07/2021 10:43:14 AM","2021-07-05T23:59:35","Defect","Ship Staff","Ship Staff Insp.","ODME Controller Keyboard unit (Membrane) buttons are hard to operate.","Critical Equip.","Cargo / Ballast Systems","Equipment Related","6.13","Low","","","New keyboard membrane received and installed, working satisfactory.","2021-11-05T23:59:35","DJAG210140","Completed","2021-07-19T23:59:35","No","No","No","Internal",""]
[null,null,null,22195,null,"30_Mon Nov 01 2021 06:27:32 GMT+0000","2021-07-16T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Many man-hole doors on the Main Deck need maintenance and their handles wasted.","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.3","Medium","","","Wasted handles renewed, de-rusted and re-painted. Looks new now.","2021-11-23T23:59:35","","Completed","2021-10-23T23:59:35","No","No","No","Internal"]
[null,null,null,20688,null,"30_31/08/2021 11:00:45 PM","2021-07-16T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","IG Line on deck, rust is appearing on the piping.","Deck - Pipe / Fittings","Cargo / Ballast Systems","External Factors","11.4","Very High","","","Completed derusting & painting of IG line","2021-09-17T23:59:35","","Completed","2021-09-07T23:59:35","No","No","No","Internal",""]
[null,null,null,20689,null,"30_31/08/2021 10:47:14 PM","2021-07-16T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","C-Deck (P & S) too many rust spots on the deck.","Accommodation","General Appearance","External Factors","11.3","Medium","","","Completed Derusting & painting of C-deck outside Accommodation P & S side","2021-09-17T23:59:35","","Completed","2021-09-06T23:59:35","No","No","No","Internal",""]
[null,null,null,20690,null,"30_31/08/2021 10:49:23 PM","2021-07-16T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Under Bridge Wing (P & S) have many rust spots.","Accommodation","General Appearance","External Factors","11.8","Low","","","Completed Derusting & painting under bridge wings  P & S.","2021-09-17T23:59:35","","Completed","2021-09-10T23:59:35","No","No","No","Internal",""]
[null,null,null,20692,null,"30_31/08/2021 10:59:04 PM","2021-07-16T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Deck House aft wards, too much rust appearing.","Accommodation","General Appearance","External Factors","11.8","Low","","","Completed derusting & painting on Accommodation block forward & aft. Photos for the same will be shared on weekly maintenance report","2021-09-17T23:59:35","","Completed","2021-09-08T23:59:35","No","No","No","Internal",""]
[null,null,null,20693,null,"30_31/08/2021 11:02:24 PM","2021-07-16T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Compass Deck Signal Light Post rust appearing below the lantern base plates.","Deck - Pipe / Fittings","General Appearance","External Factors","11.8","Low","","","Planned after departure from loading port","2021-11-23T23:59:35","","Completed","2021-10-08T23:59:35","No","No","No","Internal",""]
[null,null,null,20695,null,"30_31/08/2021 10:56:48 PM","2021-07-16T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Funnel & Engine Casing, all around too much rust appearing.","Miscellaneous","General Appearance","External Factors","11.8","Low","","","Completed derusting & painting around E/R casing & Funnel casing at Zhoushan Anchorage.","2021-11-23T23:59:35","","Completed","2021-11-17T23:59:35","No","No","No","Internal",""]
[null,null,null,20696,null,"30_31/08/2021 10:36:02 PM","2021-07-16T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Many accommodation Fire Hose Boxes have too much condensation collected causing rusting.\n\n","LSA / FFA","Safety / LSA / FFA","External Factors","5.35","Medium","","","All accommodation fire hose boxes inspected & cleaned, flushed with FW","2021-08-13T23:59:35","","Completed","2021-08-10T23:59:35","No","No","No","Internal"]
[null,null,null,20697,null,"30_31/08/2021 10:38:51 PM","2021-07-16T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Gymnasium equipment all not secured against rough seas.","Accommodation","ISM Related","Industry Issue","11.13","Low","","","All loose equipments in gymnasium secured permanently","2021-07-27T23:59:35","","Completed","2021-08-20T23:59:35","No","No","No","Internal"]
[null,null,null,20698,null,"30_31/08/2021 10:51:43 PM","2021-07-16T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","M5 Mooring Winch drip tray edges have wasted. ","Deck - Mooring Machinery","Mooring","External Factors","9.14","Medium","","","Derusting & painting of M5 mooring winch drip tray completed","2021-08-08T23:59:35","","Completed","2021-08-11T23:59:35","No","No","No","Internal"]
[null,null,null,20699,null,"30_31/08/2021 11:04:34 PM","2021-07-16T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Windlass (S) the gear cover has wasted.","Deck - Mooring Machinery","General Appearance","External Factors","9.20","Medium","","","Completed derusting & painting of P & S windlass cover, same reported in Weekly report","2021-08-08T23:59:35","","Completed","2021-08-17T23:59:35","No","No","No","Internal"]
[null,null,null,20700,null,"30_20/08/2021 0:34:33","2021-07-16T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Oxy-Acetelene high pressure rubber hoses have cracks and signs of aging","E/R - Pipes/ valves & fittings","Safety / LSA / FFA","Equipment Related","5.26","Medium","","","Connecting hoses renewed.","2021-08-02T23:59:35","","Completed","2021-08-01T23:59:35","No","No","No","Internal"]
[null,null,null,20701,null,"30_20/08/2021 0:31:32","2021-07-16T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","AHU fresh air intake filter corroded","Accommodation","Structural Condn. / WT integrity ","Equipment Related","11.8","Low","","","Filter casing removed, repair and painting carried out.","2021-09-25T23:59:35","","Completed","2021-08-14T23:59:35","No","No","No","Internal"]
[null,null,null,20702,null,"30_20/08/2021 0:27:59","2021-07-16T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ER Aft bilge well top, below fwd stern seal, accumulation of water observed.","Hull & Tanks","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Aft bilge well is located slightly forward to the aft most bulkhead ( about 2 meters) Condensation water may get collected when vessel is stand still ( during ballast vayages)but will drain when vessel start moving.","2021-08-02T23:59:35","","Completed","2021-07-27T23:59:35","No","No","No","Internal"]
[null,null,null,20199,null,"30_26/07/2021 8:00:30 PM","2021-07-18T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Slight seepage of oil noticed on portside hydraulic brake piston rod. On closer inspection, observed scratch marks/ pittings on the piston rod.","Deck - Machinery,Deck - Mooring Machinery","Mooring","Equipment Related","9.2","Very High","","","New piston rod threads for mounting piston are different than the existing one. Assembled the brake hydraulic cylinder with old piston rod. Shaft seals were renewed.  The brake screw was adjusted to original marking on to the brake arm for proper tension of the brake. Brake releasing function checked by hydraulic power several times. Function is satisfactory and there is no leak from shaft seal. Job Order V-DJAG038824/22.","2022-03-23T23:59:35","DJAG210143 Received.","Completed","2022-02-24T23:59:35","No","No","No","Internal",""]
[null,null,null,20452,null,"30_Wed Aug 18 2021 03:40:00 GMT+0000","2021-07-26T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Main engine unit no 1 piston ring found stuck inside groove.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","At VIZHINJAM anchorage, Piston replaced with spare piston with new piston rings and stuffing box.","2021-07-27T23:59:35","","Completed","2021-07-27T23:59:35","No","No","No","Internal"]
[null,null,null,20453,null,"30_Wed Aug 18 2021 03:46:32 GMT+0000","2021-08-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Copper pipe carrying Grease from grease nipple to the Hoisting & lowering sheaves found crack & leaking.","Deck - Machinery","Safety / LSA / FFA","Equipment Related","5.47","Medium","","","Section of pipe replaced.","2021-08-24T23:59:35","","Completed","2021-08-24T23:59:35","No","No","No","Internal"]
[null,null,null,20454,null,"30_Wed Aug 18 2021 03:50:38 GMT+0000","2021-08-03T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Fresh Water Generator deflector plate stand sheared off.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Sstainless steel support fabicated, evaporator and condenser cleanig done. 184 choked  tubes from evaporator cleared","2021-10-24T23:59:35","","Completed","2021-09-13T23:59:35","No","No","No","Internal",""]
[null,null,null,20694,null,"30_31/08/2021 11:09:44 PM","2021-08-23T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Observed Neutralizing agent mixture seeping from flang of neutralizing line valve above pumproom top. Valve to be overhauled & inspected","Deck - Pipe / Fittings","Cargo / Ballast Systems","External Factors","11.4","Very High","","","NA line valve above pump room top overhauled. same reported in weekly maintenance report","2021-09-23T23:59:35","","Completed","2021-09-03T23:59:35","No","No","No","Internal",""]
[null,null,null,20828,null,"30_15/09/2021 5:14:13 PM","2021-08-26T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Scattered rust spots on accommodation front.","Accommodation","General Appearance","External Factors","11.8","Low","","","Completed derusting & painting of accommodation front after epproval from office. same will be reported in WK 37 deck maintenance report","2021-10-25T23:59:35","","Completed","2021-09-07T23:59:35","No","No","No","Internal"]
[null,null,null,25950,null,"30_Sat Jul 02 2022 04:03:15 GMT+0000","2021-09-07T23:59:35","Defect","Ship Staff","Ship Staff Insp.","During BWTS testing, No.1 BWTS \"Filter Fault\" alarm triggered along with \"Fault motor protection\" & \"Motor plug\" alarm.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","6.22","Medium","","","Renewed the Proximity sensor and tried out #1 Ballast Pump,  Filter functioning satisfactory.","2022-06-23T23:59:35","DJAG210155","Completed","2022-06-22T23:59:35","No","No","No","Internal"]
[null,null,null,20827,null,"30_15/09/2021 7:50:18 PM","2021-09-08T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Water seepage observed from the bonnet of a valve of deck seal sea water pipe in engine room","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Opened up the bonnet, observed it's threads are damaged. Suitable spare valve found, Valve renewed.","2021-09-23T23:59:35","","Completed","2021-09-09T23:59:35","No","No","No","Internal",""]
[null,null,null,21320,null,"30_23/09/2021 6:51:22 AM","2021-09-09T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Presentation flange of VECS manifold reducer found painted with Epoxy paint which is unacceptable at many terminals.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Inappropriate Procedure","8.41","Medium","","","Maintenance carried out on 4 nos VECS reducer flanges, paint coating removed. ","2021-09-23T23:59:35","","Completed","2021-09-16T23:59:35","No","No","No","Internal"]
[null,null,null,21319,null,"30_01/10/2021 1:07:41","2021-09-13T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Elevator cage door jumper swich (proximity switch for door open limit) malfunction.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.37","Medium","","","DJAG210151 RECEIVED ON 12 DEC 21. PROXIMITY SWITCHES REPLACED WITH NEW. JOB ORDER 561.001.00.00 // V-DJAG037414/21.","2021-12-24T23:59:35","DJAG210151","Completed","2021-12-08T23:59:35","No","No","No","Internal",""]
[null,null,null,21317,null,"30_22/09/2021 11:55:31 PM","2021-09-15T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Faulty O2 & H2S sensor for pumproom fixed gas detection system. Sensor are not responding to SPAN gas &  0-20 mA calibration. FAULT alarm is triggered on the system & unable to reset","Miscellaneous","Safety / LSA / FFA","Equipment Related","8.46","Very High","","","Annual shore service of fixed gas detection system for P/room completed at Singapore on 12 dec 2021. Faulty O2 & H2S Sensor replaced","2021-12-15T23:59:35","DJAG215049","Completed","2021-12-05T23:59:35","No","No","No","Internal",""]
[null,null,null,21316,null,"30_30/09/2021 1:28:38 PM","2021-09-20T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Slight water leak observed from the valve stem of  LT fresh water system 3- way valve","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Leak is due to material contraction as the temperature is low in LT cooler ( vessel in Norway). Awaiting change of situation before taking any action. - Leakage is stoped after some days when temperature is increased.","2021-11-23T23:59:35","","Completed","2021-10-01T23:59:35","No","No","No","Internal",""]
[null,null,null,21318,null,"30_30/09/2021 3:15:29 PM","2021-09-21T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Pump room fire alarm buzzer going on and off occasionally.","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.35","Medium","","","Investigation done. suspect the PLC malfunction. currently there is no alarm. JOB IS CLOSING AS NO ALARM APPEARED FOR THE LAST ONE MONTH","2021-11-23T23:59:35","","Completed","2021-10-22T23:59:35","No","No","No","Internal",""]
[null,null,null,21558,null,"30_15/10/2021 10:54:36 PM","2021-09-24T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Aux Engine # 3 unit no 5 & 6 fuel valves found stuck with sleeve in cylinder head.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","cylinder heads removed. fuel valve taken out with the sleeve in workshop. new sleeve and spare fuel valve used. cylinder heads pressure tested and boxed back.","2021-10-03T23:59:35","","Completed","2021-10-02T23:59:35","No","No","No","Internal"]
[null,null,null,21559,null,"30_16/10/2021 2:24:40","2021-09-24T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Atmospheric condenser steam dump valve bonnet gasket leakage","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Gasket renewed after closing the main steam stop valve and de-pressurising the lines","2021-09-27T23:59:35","","Completed","2021-09-26T23:59:35","No","No","No","Internal"]
[null,null,null,21561,null,"30_16/10/2021 2:09:34","2021-09-24T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Main engine no-4 unit  HP pipe ( fwd injector ) fuel leakage from connecting block. ","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Pipe removed, seats lapped. pipe replaced with reconditioned one. ","2021-09-27T23:59:35","","Completed","2021-09-27T23:59:35","No","No","No","Internal"]
[null,null,null,21560,null,"30_16/10/2021 2:15:53","2021-09-26T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Main lube oil Maotti filter elements found broken while cleaning ( 40 out of 60 discs are damaged in full flow chamber)","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Filter replaced with spare discs, one set will be ordered to keep as spare","2021-09-27T23:59:35","","Completed","2021-09-27T23:59:35","No","No","No","Internal"]
[null,null,null,21562,null,"30_16/10/2021 2:21:19","2021-09-26T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Composite boiler furnace side tubes found choked. ( about 80 numbers) ","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Internal cleaning carried out. cleared all the tubes from inside with iron rod, later cleaned with water","2021-09-27T23:59:35","","Completed","2021-09-27T23:59:35","No","No","No","Internal"]
[null,null,null,21563,null,"30_16/10/2021 2:27:30","2021-10-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Main engine SFF filter back pressure alarm appeared","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Filtter renewed","2021-10-03T23:59:35","","Completed","2021-10-01T23:59:35","No","No","No","Internal"]
[null,null,null,21564,null,"30_15/10/2021 10:41:42 PM","2021-10-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","ME JCW pump #1 breaker tripped and 440 low insulation alarm came.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.37","Medium","","","Motor insulation checked found zero. motor opened for inspection, winding found burnt. Motor replaced with spare motor for FWG ejector pump as both were having same specification. Breaker main contactors also renewed as movement of contacts found slugish.","2021-10-03T23:59:35","","Completed","2021-10-02T23:59:35","No","No","No","Internal"]
[null,null,null,21554,null,"30_15/10/2021 11:02:26 PM","2021-10-03T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Vaccum toilet vaccum pressure switch occational mal-function.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Vaccum toilet vaccum/pressure switch was occasionally mal-functioning. The pressure switch contacts were checked for tightness. and calibrate with pressure calibrator. Tested multiple times on vacuum toilet system, function is satisfactory. DJAG210161 received and kept spare for future use. PMS Job order V-DJAG038727/22.","2022-02-21T23:59:35","DJAG210161","Completed","2022-02-14T23:59:35","No","No","No","Internal",""]
[null,null,null,21555,null,"30_15/10/2021 2:35:21 AM","2021-10-05T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Auto-Pilot course change knob (Set/Lock) on bridge panel developed abnormality.","Navigation - Others","Navigation","Equipment Related","4.7","High","","","Fault rectified by service technician at Singapore on 12 Dec 2021. No spares required/consumed by service engineer.","2021-12-18T23:59:35","DJAG215042","Completed","2021-12-05T23:59:35","No","No","No","Internal",""]
[null,null,null,21556,null,"30_15/10/2021 10:49:36 PM","2021-10-07T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Aux engine no 1, unit no 1 & 5 fuel valves found stuck with sleeve in cylinder head during fuel valve overhaul","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Sleeves detached forcibilly from injector body. had to discard old sleeves 4 nos, new sleeve order placed. Currently no issues witht the injectors. RO inplace & closing the defect","2021-11-23T23:59:35","DJAG210142","Completed","2021-11-07T23:59:35","No","No","No","Internal",""]
[null,null,null,21557,null,"30_15/10/2021 4:37:58 PM","2021-10-08T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Hydraulic pipe for VRCS are corroded at many locations at support brackets & 'U' Clamps. Teflon sheet on clamps & Pipe supports are damaged due to overtightness leading to onset of corrosion on hydraulic pipelines","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","11.4","Very High","","","Maintenance of Hydraulic pipelines completed, same reported in weekly work done reports. Teflon sheet on pipe support bracket & 'U' clamps been replaced for each sections.","2021-12-08T23:59:35","","Completed","2021-11-15T23:59:35","No","No","No","Internal",""]
[null,null,null,22190,null,"30_25/10/2021 10:46:42 PM","2021-10-11T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Bosun store bilge eductor inoperative even at 12 bar driving pressure","Deck - Pipe / Fittings","Emgcy. Systems","Equipment Related","8.61","Medium","","","Eductor system observed operative at 11 Bar pressure. Capable to empty the bilges in 2.5-3.0 minutes time.","2022-02-21T23:59:35","","Completed","2022-02-07T23:59:35","No","No","No","Internal",""]
[null,null,null,22191,null,"30_29/10/2021 5:08:24 PM","2021-10-11T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Soot collecting tank internal seperation plate corrotion damage","Hull & Tanks","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Hot work permission taken, weld repair carried out inside, surface preparation done, epoxy coating done.","2021-11-08T23:59:35","","Completed","2021-10-27T23:59:35","No","No","No","Internal",""]
[null,null,null,22192,null,"30_25/10/2021 10:40:30 PM","2021-10-14T23:59:35","Defect","Ship Staff","Ship Staff Insp.","ODME printer erratic. Speed of the printer motor is unusualy fast & the prined readings are unreadable","Miscellaneous","Cargo / Ballast Systems","Equipment Related","6.13","Low","","","New printer installed during annual shore based service of ODME at Singapore on 12 Dec 2021.","2021-12-14T23:59:35","DJAG210208","Completed","2021-12-05T23:59:35","No","No","No","Internal",""]
[null,null,null,22193,null,"30_25/10/2021 10:16:05 PM","2021-10-18T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Embarkation light for forward liferaft not working","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.31","High","","","New embarkation light for forward liferaft received at Singapore on 12 Dec 2021 & same installed","2021-12-18T23:59:35","DJAG210168","Completed","2021-12-05T23:59:35","No","No","No","Internal",""]
[null,null,null,26185,null,"30_Sun Jul 17 2022 04:37:21 GMT+0000","2021-10-22T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Anemometer showing erratic readings.","Navigation - Others","Navigation","Equipment Related","4.7","High","","","Renewed Anemometer with new Spare received.","2022-07-24T23:59:35","DJAG210172","Completed","2022-06-27T23:59:35","No","No","No","Internal"]
[null,null,null,22563,null,"30_15/11/2021 1:55:47","2021-10-29T23:59:35","Defect","Ship Staff","Ship Staff Insp.","ECR A/C system gas pressure observed reducing slowly over a period of 1 month, indicating minute leakage,","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","System isolated, all the remaining gases collected in recovery bottles, complete pressure test of condenser and all system along with pipe lines and pressure gauges carried out. Pressure drop around with condenser connections, same repaired, system vacuum test done for 8 hours, gas filled, system is working satisfactorily now.","2021-11-13T23:59:35","","Completed","2021-11-03T23:59:35","No","No","No","Internal"]
[null,null,null,22561,null,"30_13/11/2021 9:08:31 PM","2021-11-03T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Cable Sheathing damage observed underneath Ballast tank gauging signal line on deck, due to chafeing with support bracket.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","11.4","Very High","","","Teflon sheet placed between the support bracket & underside of ballast signal line hoses to prevent chafing damage.","2021-12-03T23:59:35","","Completed","2021-11-17T23:59:35","No","No","No","Internal",""]
[null,null,null,22562,null,"30_13/11/2021 9:05:13 PM","2021-11-06T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Breather valve on mast riser observed leaking due to damaged diapdragm.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.19","High","","","Diaphragm for mastriser breather valve replaced with spares received at Singapore on 12 Dec 2021.","2022-01-06T23:59:35","DJAG210124","Completed","2021-12-07T23:59:35","No","No","No","Internal",""]
[null,null,null,22714,null,"30_01/12/2021 14:13:49","2021-11-12T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Steam pipe flange ( fuel tank heating line) in purifier room have  leakage, Gasket need to be renewed.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Gasket renewed at anchorage after closing the steam stop vlave and shutting down the steam supply.","2021-11-23T23:59:35","","Completed","2021-11-16T23:59:35","No","No","No","Internal"]
[null,null,null,22713,null,"30_26/11/2021 3:14:25 PM","2021-11-13T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Composite boiler FO pressure regulating valve spring found damaged.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Composite boiler fuel oil pressure regulating valve spring found damaged. Fuel oil pressure regulating valve replaced with the new spare. Opening pressure adjusted to 17.1 bar, as per manual. Composite boiler tried out, found working satisfactory. PMS Job V-DJAG038728/22.","2022-02-21T23:59:35","DJAG210196","Completed","2022-02-14T23:59:35","No","No","No","Internal",""]
[null,null,null,22715,null,"30_01/12/2021 13:59:24","2021-11-14T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Aux engine-2, unit-5 exhaust gas sensor malfunction.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Sensor renewed.","2021-11-18T23:59:35","","Completed","2021-11-15T23:59:35","No","No","No","Internal"]
[null,null,null,23856,null,"30_01/02/2022 12:19:43 PM","2021-11-20T23:59:35","Observation","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","Random/Unannounced shore-based drug test had exceeded more than one year from the previous test carried out on 14-Oct-2020","Miscellaneous","Crew Management","External Factors","3.8","Very High","","","Due to the trade pattern, vessel could not timely carry out the annual shore based test. Vessel completed annual shore based D&A test at Qingdao, China on 01 Dec 2021.","2021-12-20T23:59:35","","Completed","2021-11-24T23:59:35","No","No","No","External"]
[null,null,null,22716,null,"30_01/12/2021 14:26:02","2021-11-20T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Steering gear hydraulic lock alarm appears at about 20-30 deg port side movement.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Upon investigation, one of the 'proxy switches' found not functioning. Same replaced with spare switch. Issue is solved.","2021-11-23T23:59:35","","Completed","2021-11-21T23:59:35","No","No","No","Internal"]
[null,null,null,23099,null,"30_14/12/2021 7:47:31 PM","2021-12-05T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Hospital house-keeping is poor and long bath is dirty.","Accommodation","General Appearance","Behaviour Based","11.15","Low","","","Thorough cleaning of Hospital & long bath completed. Same reported in Weekly workdone report.","2021-12-12T23:59:35","","Completed","2021-12-10T23:59:35","No","No","No","Internal",""]
[null,null,null,23101,null,"30_14/12/2021 7:50:31 PM","2021-12-05T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Forward Bosun Store, No.2 Hyd Pump is leaking hydraulic oil.","Deck - Mooring Machinery","Mooring","Equipment Related","11.12","Low","","","No 2 fwd Hyd pump checked for leakage by running it in Work pressure it was observed that oil leak is from delivery valve gland.Job was planned,system drain ball valve removed from place and overhualed in the workshop.Valve fitted back and system tried out.Presntly system running normal without any leakage.Job reported as unplanned V-DJAG037535/21.","2022-02-05T23:59:35","","Completed","2021-12-13T23:59:35","No","No","No","Internal",""]
[null,null,null,23102,null,"30_14/12/2021 7:54:21 PM","2021-12-05T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Main Deck lamp post & its vertical ladder at No.4 COT already corroded.","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.1","High","","","Derusting & painting of vertical ladder of deck lamp post completed","2022-02-05T23:59:35","","Completed","2021-12-20T23:59:35","No","No","No","Internal",""]
[null,null,null,23103,null,"30_14/12/2021 7:57:12 PM","2021-12-05T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Cargo cross-over piping after valve, OD-307, may be holed already.","Deck - Pipe / Fittings","General Appearance","External Factors","11.4","Very High","","","Completed maintenance of Cross-over pipeline, valves & all associated fittings. Reported in weekly work done report","2021-12-19T23:59:35","","Completed","2021-12-08T23:59:35","No","No","No","Internal",""]
[null,null,null,23104,null,"30_14/12/2021 8:00:47 PM","2021-12-05T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Main Deck forward of midship, many VRC tubing and WBT gas sampling tubing shield & support bar already corroded.","Deck - Pipe / Fittings","General Appearance","External Factors","11.5","Medium","","","Completed maintenance of all shield & support bar of VRC tubing, WBT gas sampling tubing etc forward of manifold.","2022-02-05T23:59:35","","Completed","2021-12-31T23:59:35","No","No","No","Internal",""]
[null,null,null,23105,null,"30_14/12/2021 8:03:10 PM","2021-12-05T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Many rusty spots on the Main Deck below all the cargo piping supports.","Deck - Pipe / Fittings","General Appearance","External Factors","11.3","Medium","","","Completed Derusting & painting work of main deck below cargo piping support. Detailed pictures reported in Weekly work done report dated: 13 Feb 2022","2022-02-05T23:59:35","","Completed","2022-02-04T23:59:35","No","No","No","Internal",""]
[null,null,null,23106,null,"30_14/12/2021 8:06:12 PM","2021-12-05T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Compass Deck Radar Mast rust appearing below the lantern base plates, ladder, etc.","Miscellaneous","General Appearance","External Factors","11.8","Low","","","Completed Cosmetic maintenance of Main mast, lantern base plate, ladder etc.\n\nSame will be reported in Weekly work done report","2022-02-05T23:59:35","","Completed","2021-12-23T23:59:35","No","No","No","Internal",""]
[null,null,null,23108,null,"30_15/12/2021 12:31:49 PM","2021-12-05T23:59:35","Defect","Ship Staff","Ship Staff Insp.","HP Air hose from air bottle to manifold found in poor condition. Same to be replaced","LSA / FFA","Safety / LSA / FFA","External Factors","5.28","Very High","","","New HP hosed received at Singapore on 12 Dec 2021. Same replaced","2022-01-05T23:59:35","","Completed","2021-12-09T23:59:35","No","No","No","Internal",""]
[null,null,null,26186,null,"30_Sun Jul 17 2022 04:42:31 GMT+0000","2021-12-05T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","AHU Fresh Air Intake Filter already corroded.","Accommodation","General Appearance","Equipment Related","11.8","Low","","","New AHU filters received and renewed.","2022-07-24T23:59:35","DJAG220011","Completed","2022-07-04T23:59:35","No","No","No","Internal"]
[null,null,null,25951,null,"30_Sat Jul 02 2022 04:06:48 GMT+0000","2021-12-05T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Main Engine Top Bracing forward, No.2 is leaking.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Presently Top bracing unit #2 is not leaking, it is under close observation. If it starts leaking we will carry out overhauling as vessel received the spares.","2022-06-23T23:59:35","DJAG220007","Completed","2022-06-17T23:59:35","No","No","No","Internal"]
[null,null,null,23267,null,"30_30/12/2021 5:17:26 PM","2021-12-10T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Close-up inspection & maintenance of stay wires of main mast. Anti corrosive coating to be applied on stay wires. Also P & S Navigation light post stay wires to be renewed.","Miscellaneous","General Appearance","External Factors","11.8","Low","","","Maintenance of stay wires of main mast completed.  P & S Navigation light post stay wires renewed and anti corrosive coating applied..","2022-01-24T23:59:35","","Completed","2022-12-01T23:59:35","No","No","No","Internal",""]
[null,null,null,26677,null,"30_Sun Sep 04 2022 10:34:09 GMT+0000","2021-12-20T23:59:35","Defect","Ship Staff","Ship Staff Insp.","AHU room accommodation aircon fresh air intake gas detection sensor is not responding to calibration. Sensor is defective.","Accommodation","Safety / LSA / FFA","Equipment Related","5.1","Very High","","","Now Sensor is working and activating the alarm","2022-08-24T23:59:35","DJAG220012","Completed","2022-08-23T23:59:35","No","No","No","Internal"]
[null,null,null,25952,null,"30_Sat Jul 02 2022 04:09:41 GMT+0000","2021-12-20T23:59:35","Defect","Ship Staff","Ship Staff Insp.","ECR aircon # 2 is non-operational due to air intake temperature sensor defective.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Renewed air intake temp sensor with new spares received, now working satisfactory.","2022-06-23T23:59:35","DJAG220006","Completed","2022-06-12T23:59:35","No","No","No","Internal"]
[null,null,null,23269,null,"30_28/12/2021 1:18:10","2021-12-20T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Aux Engine# 2, units 2, 3&4 fuel valves are found stuck in cylinder head, can`t pull out.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","AE# 2, unit # 2 injector was pulled out and replaced with overhauled spare. Unit #3&4 cylinder heads dismounted. Bush for fuel valve were replaced for unit # 3&4. Both units cylinder heads were monted back with overhauled injector. Postponed jobs V-DJAG022478/19 // V-DJAG022479/19 // V-DJAG022480/19 were completed.","2022-02-21T23:59:35","DJAG210142","Completed","2022-02-17T23:59:35","No","No","No","Internal",""]
[null,null,null,23270,null,"30_28/12/2021 1:23:37","2021-12-20T23:59:35","Defect","Ship Staff","Ship Staff Insp.","LT cooler temperature control 3-way valve has minor leak from spindle sahft seal. Seal to be replaced.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","",".SYSTEM ISOLATED,LOAD ON AE REDUCED,CONTROLLER DISMANTLE ,ROTOR GLAND REMOVED AND O-RING RENEWED.\n\nREPORTED IN PAL AS UNPLANNED JOB NO-V-DJAG037880/22.PO RAISED FOR SPARE.","2022-02-21T23:59:35","DJAG220008","Completed","2022-01-04T23:59:35","No","No","No","Internal",""]
[null,null,null,23271,null,"30_28/12/2021 8:30:53 PM","2021-12-20T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Port Life Boat engine sprinkler pump coupling pad is crushed/cracked. To be replaced.","LSA / FFA","Safety / LSA / FFA","Equipment Related","4.27","High","","","Spider coupling is replaced with new spare. Life boat engine running test was carried out, no abnormal sound or vibration from coupling. Satisfactory. PMS Job order V-DJAG038729/22.","2022-02-21T23:59:35","DJAG220003","Completed","2022-02-14T23:59:35","No","No","No","Internal",""]
[null,null,null,23272,null,"30_28/12/2021 1:29:47","2021-12-20T23:59:35","Defect","Ship Staff","Ship Staff Insp.","A deck light on top of stbd side mid-ship store is causing low insulation","Elect. Mach. & Equip.","Navigation","Equipment Related","10.38","Medium","","","220VAC low insulation was detected from a deck flood light on top of stbd mid-ship store. Faulty cable 3-core, 5 meter in length from JB to the light fitting was renewed. Insulation improved from 2 Mohm to 500 Mohm. PMS JOB ORDER: 893.001 // \n\nV-DJAG037938/22","2022-01-24T23:59:35","","Completed","2022-01-01T23:59:35","No","No","No","Internal",""]
[null,null,null,23274,null,"30_01/01/2022 6:43:32","2021-12-20T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Deck foam pump has slight leakage from mechanical seal. Mechanical seal needs replacement","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.33","High","","","Mechanical seal  renewed after taking office approval.RO rasied for the same.","2022-01-24T23:59:35","DJAG220001-FIRE FIGHTING SYSTEMS W/FOAM","Completed","2021-12-29T23:59:35","No","No","No","Internal",""]
[null,null,null,23275,null,"30_28/12/2021 1:13:43","2021-12-20T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Anchor Windlass # 2 gear oil appearance is found emulsified. Onboard analysis was carried out for both windlass and three mooring winches, result as follows: W1-0.27%, W2-0.55%, M1-0.16%, M2-0.10%, M3-0.26%. W1 &W2 gear oil renewed. M1,M2 & M3 oil is to be renewed.","Deck - Mooring Machinery","Mooring","Equipment Related","9.14","Medium","","","Onboard analysis was carried out for both windlass and three mooring winches, result as follows: W1-0.27%, W2-0.55%, M1-0.16%, M2-0.10%, M3-0.26%. MW1, MW2, M3 ,M4 & M5 oil renewed. PMS 439 // JOB ORDER V-DJAG037714/22 .","2021-12-23T23:59:35","-","Completed","2021-12-20T23:59:35","No","No","No","Internal"]
[null,null,null,23276,null,"30_01/01/2022 6:33:57","2021-12-20T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Composite boiler main engine exhaust gas side 10 in no. tubes found chocked.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Main engine exhaust side water washing was carried out. 10 in nos. tubes were found chocked with hard carbon/soot. All chocked tubes were cleared by digging manually. Now all tubes on exhaust side are clear for passage of main engine exhaust.Job reported in PMS 646.005.00.00 // JO number V-DJAG037694/21.","2021-12-24T23:59:35","","Completed","2021-12-21T23:59:35","No","No","No","Internal"]
[null,null,null,26187,null,"30_Sun Jul 17 2022 04:45:00 GMT+0000","2022-01-10T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Diail type float gauge for grey water double bottom tank in engine room found defective.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Renewed Float with new spares received.","2022-07-24T23:59:35","DJAG220020","Completed","2022-07-05T23:59:35","No","No","No","Internal"]
[null,null,null,25768,null,"30_Fri Jun 24 2022 03:08:18 GMT+0000","2022-01-10T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Fish room high temperature alarm triggered. Controller was found defective during fault finding.","Accommodation","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Working controller was cannibalized from wet garbage locker and fitted on Fish Room. Fish room cooling system is fully operational. Wet garbage locker cooling system new controller spare received and fitted back.","2022-06-08T23:59:35","DJAG220015","Completed","2022-06-08T23:59:35","No","No","No","Internal"]
[null,null,null,23741,null,"30_31/01/2022 6:08:57 PM","2022-01-11T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Engine room alarm monitoring system ROS-2 LCD monitor has lost display, screen is blank.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Replaced with new display LCD/TN MD22 MK3, LED backlight, 16.9, 1920 x 1080, Input 90-264 VAC. Tested after replacement and put it into service found in order. Job order V-DJAG038730/22.","2022-02-21T23:59:35","DJAG220019","Completed","2022-02-14T23:59:35","No","No","No","Internal",""]
[null,null,null,26188,null,"30_Sun Jul 17 2022 04:47:39 GMT+0000","2022-01-12T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Main engine JCW pump No.2 giving abnormal sound and vibration during running","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Pump Overhauled with spares received and now working well.","2022-01-12T23:59:35","DJAG220023","Completed","2022-07-08T23:59:35","No","No","No","Internal"]
[null,null,null,23857,null,"30_14/02/2022 9:28:46 AM","2022-01-20T23:59:35","Non Conformity","Owner / Marine / Tech. Suptd.","ISM Audit","1.08.23: Copies of Statutory Certificates Displayed (SOLAS I REG. 16) - Copies were not displayed.","Miscellaneous","Cert. & Docu.","Inappropriate Procedure","2.1","Very High","","","ALL STATUTORY CERTIFICATES COPIES PRINTED AND POSTED ON NOTICE BOARD OUTSIDE MASTER'S CABIN.","2022-04-19T23:59:35","","Completed","2022-01-30T23:59:35","No","No","No","Internal"]
[null,null,null,23858,null,"30_14/02/2022 9:40:36 AM","2022-01-20T23:59:35","Observation","Owner / Marine / Tech. Suptd.","ISM Audit","Meat room + Veg room - sighted oversized plastic bins which are overlapping the shelves & hence anti-roll strips cannot be placed - consider realigning the plastic trays so that anti-roll strips can be placed back ","Miscellaneous","General Appearance","Inappropriate Procedure","11.13","Low","","","All referigerated spaced cleaned & re arranged. Anti-roll stripes placed in position after arranging the stores.","2022-04-19T23:59:35","","Completed","2022-02-05T23:59:35","No","No","No","Internal"]
[null,null,null,23859,null,"30_14/02/2022 10:23:45 AM","2022-01-20T23:59:35","Observation","Owner / Marine / Tech. Suptd.","ISM Audit","windlass - mooring wires to be reeved in symmetrically after each mooring operation - this will prevent the wire getting jammed  when being heaved up at a berth when under tension - then when casting off the berth it becomes very difficult to release the wire which is jammed.  ","Deck - Mooring Machinery","Mooring","Inappropriate Procedure","9.1","Low","","","All mooring wires re arranged evenly on the storage drum","2022-04-19T23:59:35","","Completed","2022-02-07T23:59:35","No","No","No","Internal"]
[null,null,null,23860,null,"30_14/02/2022 9:32:49 AM","2022-01-20T23:59:35","Observation","Owner / Marine / Tech. Suptd.","ISM Audit","Cargo over board seal - In addition - recommend also place a seal on the extended spindle of the valve (iwo split pin). This will ensure that the valve cannot be operated by removing the valve wheel ","Deck - Pipe / Fittings","Cargo / Ballast Systems","Inappropriate Procedure","6.4","High","","","Securing/locking arrangement improvised for cargo overboard. Security seal placed on the extended spindle of the valve iwo split pin to ensure the calve cannot be operated without breaking the seal.","2022-04-19T23:59:35","","Completed","2022-02-07T23:59:35","No","No","No","Internal"]
[null,null,null,23743,null,"30_31/01/2022 7:24:47 AM","2022-01-23T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Observed Crack on the casing of Portable Spill Pump used for rapid disposal of oil at the aft end of the main deck.","Deck - Pipe / Fittings","MARPOL Related","Equipment Related","6.3","Low","","","Spare Diaphragm pump was installed in place of Portable spill pump with damaged casing.","2022-04-23T23:59:35","","Completed","2022-02-15T23:59:35","No","No","No","Internal",""]
[null,null,null,23854,null,"30_14/02/2022 11:48:03 AM","2022-01-31T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Echo Sounder repeater in the Port Side Bridge wing console not showing proper digital readings. Suspect some of the segment LED’s are probably fused.","Navigation - Echo Sounder / Speed Log","Navigation","Equipment Related","4.19","Low","","","Service technician attended at Singapore on 17th Feb 2022. He replaced the old unit with new display unit. The new unit dimensions are different from old unit. Ship staff fabricated securing plate for the new unit and fitted in place.","2022-04-29T23:59:35","","Completed","2022-02-16T23:59:35","No","No","No","Internal",""]
[null,null,null,26678,null,"30_Sun Sep 04 2022 10:36:17 GMT+0000","2022-02-05T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Pressure transmitter for APT BWTS filter inlet observed faulty. PT to be replaced.","Miscellaneous","Cargo / Ballast Systems","Equipment Related","6.21","High","","","Renewed the received Spare Sensor.","2022-09-23T23:59:35","DJAG220147","Completed","2022-08-24T23:59:35","No","No","No","Internal"]
[null,null,null,30544,22873,"30_Wed Mar 08 2023 15:37:38 GMT+0800","2022-03-03T23:59:35","Observation","Ship Staff","Ship Staff Insp.","UKC calculation sheet should be included with the Pilot Information card","Navigation - Others","Navigation","Inappropriate Procedure","4.1","High","","","OOWs must cross check  that Pilot information card and  UKC sheets are also included while presenting to the pilot. Master to ensure complete documentation is available to the pilot.","2023-06-03T23:59:35","","Completed","2022-03-03T23:59:35","No","No","No","Internal"]
[null,null,null,30545,78669,"0_Wed Mar 08 2023 15:40:05 GMT+0800","2022-03-03T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Vessel's positions from previous passages must be removed from the charts on the ECDIS while preparing the route. ","Navigation - Others","Navigation","Knowledge Based","4.14","Very High","","","Past positions deleted from the route. 2nd officer instructed to ensure that past positions are removed whilst planning the route. Other OOWs instructed to  cross check.","2022-06-03T23:59:35","","Completed","2022-03-03T23:59:35","No","No","No","Internal"]
[null,null,null,24673,null,"30_28/03/2022 11:21:07 PM","2022-03-13T23:59:35","Defect","Ship Staff","Ship Staff Insp.","For the past few days, the speed log is showing erratic readings. The speed values drops and varies between -1k to 9k. The system was rebooted few times. Immediately after powering on, the log sometimes steadies to correct value for few hours and then becomes erratic.","Navigation - Echo Sounder / Speed Log","Navigation","External Factors","4.7","High","","","The fore peak tank was de-ballasted and an entry was made to the speed log space for inspection. It was noticed that the transducer got lifted up by 5 cm due to slack bolt on the clamp. This was the probable cause of erratic log speed values. The transducer was removed and cleaned with clean cloth as adviced; however there were no barnacles on tip. \n\n\n\nThe transducer was fitted back in order; attention was paid to its orientation. Presently the log speed value is correct and consistent.","2022-03-24T23:59:35","","Completed","2022-03-16T23:59:35","No","No","No","Internal"]
[null,null,null,25327,null,"30_06/05/2022 10:59:08 PM","2022-04-23T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Refrigerant gas detection system has following defects: \n\n(I) No.2 AC detector not working.\n\n(II) Local panel on E/R 2nd deck indication lights are not working. \n\nIII) Galley AC unit, meet and fish room detectors are showing false alarm.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","11.17","Low","","","Troubleshooting carried out and made system operational","2022-10-24T23:59:35","","Completed","2022-09-07T23:59:35","No","No","No","Internal",""]
[null,null,null,30549,91974,"30_Wed Mar 08 2023 17:01:22 GMT+0800","2022-05-19T23:59:35","Observation","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","The SMS required that the location of wires be changed to other winches, every 5 years when the end-to-end change was done. While there were records of end-to-end process having been done after 5 years in 2020, there was no evidence that the location of wires had been changed to other winches to help shift the contact points.","Deck - Mooring Machinery","Mooring","Inappropriate Procedure","9.4","High","","","A revised mooring line matrix was updated for records. This was verified and confirmed for actual completion of job by re-checking the tags and markings on mooring lines onboard in comparison to the original location of lines prior to July 2020. A briefing of all\nofficers and crew was carried out regarding proper record keeping and through verification of records for the job completed prior to their joining. Any discrepancy noted to be brought forward for verification and changes if required need to be notified to the office. This observation has been circulated to the fleet for ship staff awareness\nand compliance. Company SMS requirement is shared within the fleet for verification on board. Latest mooring line matrix to be sent to the office with correct location of mooring wires for confirmation.","2022-07-18T23:59:35","","Completed","2022-06-02T23:59:35","No","No","No","External"]
[null,null,null,25453,null,"30_Wed Jun 01 2022 02:48:22 GMT+0000","2022-05-24T23:59:35","Defect","Ship Staff","Ship Staff Insp.","NO.2 Steering Gear Janney Pump has a minor leak from by-pass valve flange, transfer valve spindle and pump end flange.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","O'ring renewed by technicians in DD","2023-02-04T23:59:35","DJAG225062","Completed","2023-02-10T23:59:35","No","No","No","Internal","Extended target date to 31st OCT 2022. We are waiting your investigation report."]
[null,null,null,26432,null,"30_Fri Aug 05 2022 03:13:46 GMT+0000","2022-06-08T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Windlasses & Mooring Winches and their operating platform have too many rusty spots.","Deck - Mooring Machinery","General Appearance","Equipment Related","9.14","Medium","","","Started doing maintenance with Hydro blaster.","2022-08-08T23:59:35","","Completed","2022-07-16T23:59:35","No","No","No","Internal"]
[null,null,null,26433,null,"30_Fri Aug 05 2022 03:15:44 GMT+0000","2022-06-08T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","FPT air vent and manhole cover need buffing & new paint.","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.7","High","","","Started doing maintenance with Hydro blaster","2022-08-08T23:59:35","","Completed","2022-07-16T23:59:35","No","No","No","Internal"]
[null,null,null,25953,null,"30_Sat Jul 02 2022 04:15:12 GMT+0000","2022-06-08T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","(P & S) Provision Crane oil level glass are already corroded.","Deck - Machinery","General Appearance","Equipment Related","8.5","Very High","","","Renewed both the Level glasses with received new spares.","2022-09-08T23:59:35","","Completed","2022-06-14T23:59:35","No","No","No","Internal"]
[null,null,null,25954,null,"30_Sat Jul 02 2022 04:18:15 GMT+0000","2022-06-08T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","2E, 4E and ETO don’t have a proper daily hard cover workbook so there is no record of their machinery history.","Documentation","Cert. & Docu.","Human Error","10.12","Very High","","","Started maintaining the record books.","2022-06-23T23:59:35","","Completed","2022-06-18T23:59:35","No","No","No","Internal"]
[null,null,null,25960,null,"30_Sat Jul 02 2022 04:49:58 GMT+0000","2022-06-08T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Many Cargo Oil Tanks’ opening, their hatch cover & coaming are rusting.","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.6","Medium","","","Completed Derusting & painting","2022-09-25T23:59:35","","Completed","2022-09-25T23:59:35","No","No","No","Internal","Extended target date to 30th SEP 2022. Revert job plan, progress and rectification in your weekly deck maintenance reporting to office."]
[null,null,null,26597,null,"30_Fri Aug 19 2022 02:41:24 GMT+0000","2022-06-08T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Funnel aft side, Engine Casing port side, Emergency Generator Room exterior at entrance, have many scattered corroded spots and rusty weeping. Accommodation exterior stairway railings need buffing & re-paint.","Hull & Tanks","General Appearance","Equipment Related","11.8","Low","","","Started doing maintenance.","2022-08-08T23:59:35","","Completed","2022-08-02T23:59:35","No","No","No","Internal"]
[null,null,null,26598,null,"30_Fri Aug 19 2022 02:43:28 GMT+0000","2022-06-08T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Many portions of shipside railings are rusting, need buffing & re-painting.","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.3","Medium","","","Started doing maintenance with Hydro blaster.","2022-08-08T23:59:35","","Completed","2022-07-22T23:59:35","No","No","No","Internal"]
[null,null,null,26679,null,"30_Sun Sep 04 2022 10:38:20 GMT+0000","2022-06-11T23:59:35","Defect","Ship Staff","Ship Staff Insp.","PA system not working.","Elect. Mach. & Equip.","Communication","Equipment Related","10.37","Medium","","","Contacts of Mic Cleaned and now it is working well.",null,"","Completed","2022-09-11T23:59:35","No","No","No","Internal"]
[null,null,null,30546,41497,"30_Wed Mar 08 2023 16:26:21 GMT+0800","2022-07-06T23:59:35","Observation","Ship Staff","Ship Staff Insp.","2 Nos. Cylinder Shapes found worn out.","Navigation - Others","Navigation","Equipment Related","4.7","High","","","Cylinder Shapes repaired as required.  All officers briefed regarding importance of regular inspection / monitoring of Bridge equipment. Any shortcoming to be immediately reported so as to be rectified on priority basis. ","2022-10-05T23:59:35","","Completed","2022-07-06T23:59:35","No","No","No","Internal"]
[null,null,null,30547,82509,"0_Wed Mar 08 2023 16:28:57 GMT+0800","2022-07-06T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Few Watchkeeping entries missing in GMDSS Log book. ","Navigation - GMDSS & Communication","Navigation","Knowledge Based","4.23","High","","","All officers briefed regarding importance of record keeping and log books entries updated every watch. Proper entries being made and log book updated every watch. Regular inspection of log books to be made by senior officers to ensure compliance.","2022-10-05T23:59:35","","Completed","2022-07-06T23:59:35","No","No","No","Internal"]
[null,null,null,30548,21704,"0_Wed Mar 08 2023 16:31:00 GMT+0800","2022-07-06T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Weather Information not detailed in course recorder at end of every watch.","Navigation - Others","Navigation","Knowledge Based","4.7","High","","","All officers briefed regarding importance of record keeping and log entries maintained every watch. Records being maintained as per requirements. Regular inspection of log records to be made by senior officers to ensure compliance.","2022-10-05T23:59:35","","Completed","2022-07-06T23:59:35","No","No","No","Internal"]
[null,null,null,26434,null,"30_Fri Aug 05 2022 03:17:46 GMT+0000","2022-07-14T23:59:35","Observation","Ship Staff","Ship Staff Insp.","ME Jacket water Heater Flange leaking .","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Renewed the damaged Gasket, tested and working satisfactory","2022-07-29T23:59:35","","Completed","2022-07-21T23:59:35","No","No","No","Internal"]
[null,null,null,26680,null,"30_Sun Sep 04 2022 10:40:33 GMT+0000","2022-08-11T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Echo Sounder Forward transducer not showing any reading on the Display.","Navigation - Echo Sounder / Speed Log","Navigation","Equipment Related","4.25","Low","","","Service Engineer attended at Singapore on 22 Aug 22 and rectified the problem","2022-08-24T23:59:35","DJAG225031","Completed","2022-08-15T23:59:35","No","No","No","Internal"]
[null,null,null,26681,null,"30_Sun Sep 04 2022 10:49:52 GMT+0000","2022-08-17T23:59:35","Defect","Ship Staff","Ship Staff Insp.","#3 Aux Engine HT Cooling Fresh Water Pump is slightly leaking from Tell tale hole.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Overhauled the Pump and changed the Mechanical Seal.","2022-09-23T23:59:35","","Completed","2022-08-25T23:59:35","No","No","No","Internal",""]
[null,null,null,26854,null,"30_Sat Sep 17 2022 01:29:51 GMT+0000","2022-08-18T23:59:35","Observation","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","VDR on Bridge was giving alarm for Float free Capsule \" Unable to record, Unit to be checked\"","Navigation - VDR / BNWAS","Navigation","Equipment Related","4.7","High","","","MARIAPPS Service Engineer Attended and renewed the Unit","2022-09-15T23:59:35","DJAG225051","Completed","2022-08-18T23:59:35","No","No","No","External"]
[null,null,null,26855,null,"30_Sat Sep 17 2022 01:34:42 GMT+0000","2022-08-18T23:59:35","Observation","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","Around 50 % of Grating on midship manifold (Both side) were Observed with paint peeled off and rusted.","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.6","Medium","","","Port side Manifold grating & Stbd side Derusting & painting completed.","2022-09-23T23:59:35","","Completed","2022-09-12T23:59:35","No","No","No","External","Revert progress and rectification in your weekly deck maintenance reporting to office."]
[null,null,null,26856,null,"30_Sat Sep 17 2022 01:40:39 GMT+0000","2022-08-30T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Stbd Windlass Control Lever is slightly leaking during Operation.","Deck - Mooring Machinery","Mooring","Equipment Related","11.4","Very High","","","Seal renewed. Unit is working without any leak at present.","2022-10-24T23:59:35","DJAG220137","Completed","2022-10-27T23:59:35","No","No","No","Internal","PO# DJAG220137 issued to maker MACGREGOR. Waiting spare readiness."]
[null,null,null,26857,null,"30_Sat Sep 17 2022 01:45:51 GMT+0000","2022-09-06T23:59:35","Defect","Ship Staff","Ship Staff Insp.","BWTS NU pump PCB not working, need to replace on receipt.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.8","Medium","","","PCB renewed, Unit is working satisfactorily.","2022-11-23T23:59:35","DJAG220191","Completed","2022-11-26T23:59:35","No","No","No","Internal","RO DJAG220191 sent on the 13th SEP 2022 to BWTS maker for quotation."]
[null,null,null,26858,null,"30_Sat Sep 17 2022 01:48:50 GMT+0000","2022-09-08T23:59:35","Defect","Ship Staff","Ship Staff Insp.","In Refrigerant leak detection system,  Galley  AC Unit PCB, Senor and Sensor Holder Faulty and #2 AC Unit Sensor Faulty.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Behaviour Based","11.17","Low","","","Spare renewed, system working satisfactorily.","2022-11-23T23:59:35","DJAG220192","Completed","2022-10-08T23:59:35","No","No","No","Internal","RO DJAG220192 sent on the 16th SEP 2022 to vendors for quotation."]
[null,null,null,30550,37601,"30_Wed Mar 08 2023 18:24:59 GMT+0800","2022-09-27T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Ship Staff Insp.","Auto pilot system not working when using steering gear pump No.2. ","Navigation - Others","Navigation","Equipment Related","4.7","High","","","System attended by service engineer at Singapore. Upon investigation found Control Box No.2 DM-DRVR PWB faulty. Same renewed and calibration carried out. Auto pilot tested and found operational on both steering gear pump.","2022-12-04T23:59:35","","Completed","2022-10-09T23:59:35","No","No","No","Internal"]
[null,null,null,30553,77617,"30_Wed Mar 08 2023 17:39:31 GMT+0800","2022-09-29T23:59:35","Observation","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","VDR Annual performance test was carried out on 12 Dec 2021, however there was no certificate of compliance of VDR annual performance test according to SOLAS Chap. V Reg. 18.8 available on board.","Documentation","Cert. & Docu.","External Factors","4.7","High","","","Certificate of compliance of VDR annual performance test according to SOLAS Chap. V Reg. 18.8 received and filed onboard.","2022-11-28T23:59:35","","Completed","2022-10-09T23:59:35","No","No","No","External"]
[null,null,null,30554,72359,"0_Wed Mar 08 2023 17:49:27 GMT+0800","2022-09-29T23:59:35","Defect","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","SAAB radar for cargo monitoring system was observed with 'no sensor alarm' of ullage and 'failure ' alarm of pressure for #2P COT at TGE unit control in CCR.","Hull & Tanks","Cargo / Ballast Systems","Equipment Related","8.12","Medium","","","New SAAB gauge received and installed. 2P COT  SAAB radar gauge made operational.","2022-12-02T23:59:35","DJAG225059","Completed","2022-10-02T23:59:35","No","No","No","External"]
[null,null,null,30558,57461,"0_Wed Mar 08 2023 17:43:43 GMT+0800","2022-09-29T23:59:35","Observation","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","Chief engineer and second engineer had joined and were relieved at the same time on 14 June 2022 without a suitable handover period.","Miscellaneous","Crew Management","External Factors","3.5","Medium","","","New Chief engineer and second engineer has sailed on sister vessel previously.\nHandover notes were of both were shared with joining engineers well in advance and same discussed over tele-conferencing.","2022-12-02T23:59:35","","Completed","2022-10-04T23:59:35","No","No","No","External"]
[null,null,null,28076,72164,"30_Tue Dec 06 2022 11:53:42 GMT+0800","2022-11-13T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Maine engine all units cooling fresh water inlet/outlet valves to renew.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","All valves renewed.","2023-02-06T23:59:35","None","Completed","2023-02-12T23:59:35","No","No","No","Internal"]
[null,null,null,30556,47629,"30_Wed Mar 08 2023 23:39:30 GMT+0800","2022-11-14T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Nav Audit / Verification","Procedures upon receipt of Distress messages (Company standing orders and SOLAS chap V Reg 33) not complied with.","Navigation - Others","Navigation","Inappropriate Procedure","4.23","High","","","Master entered the reason for not responding to Distress message in GMDSS Log Book, Vsl was 2700 NM away from Distress Position.\nD/O's were reminded to bring any Distress Communications received during their watch to Master's attention soonest, so the same can be checked and suitable actions can be taken in sufficient time.","2023-02-14T23:59:35","","Completed","2022-12-13T23:59:35","No","No","No","Internal"]
[null,null,null,30557,23803,"0_Wed Mar 08 2023 23:44:56 GMT+0800","2022-11-14T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Nav Audit / Verification","Min required UKC not mentioned in Passage plan Sheet A.","Documentation,Navigation - Others","Navigation","Knowledge Based","4.20","Very High","","","Minimum UKC required at all stages of passage plan was calculated and added in the Passage Plan Sheet A.\nMaster convened a Bridge Team Meeting the the observation was discussed with all. All D/Os were requested to be pro-active in pointing out any deviation related to Navigational procedures immediately.","2023-02-14T23:59:35","","Completed","2022-11-26T23:59:35","No","No","No","Internal"]
[null,null,null,28070,61617,"30_Fri Dec 02 2022 11:54:41 GMT+0800","2022-11-23T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","CCR steam chest gauge having error ","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.13","Medium","","","Calibrated","2023-02-22T23:59:35","","Completed","2023-02-07T23:59:35","No","No","No","Internal"]
[null,null,null,28072,61338,"30_Fri Dec 02 2022 10:44:07 GMT+0800","2022-11-23T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Spot Derusting Need to be carried out neat No.1 COT/ WBT Area","Miscellaneous","General Appearance","Inappropriate Procedure","11.3","Medium","","","Spot Derusting & painting Completed","2023-02-22T23:59:35","","Completed","2022-12-31T23:59:35","No","No","No","Internal"]
[null,null,null,28075,85475,"30_Fri Dec 02 2022 12:58:14 GMT+0800","2022-11-23T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Rust was noticed on near Crane hoisting safety limits /  Hoisting winch , drum & fittings. ","Deck - Machinery","General Appearance","Equipment Related","","","","","Derusting & painting of port & Stbd side Hose handling Crane drum fittings, hoisting winch completed","2023-02-22T23:59:35","","Completed","2023-01-03T23:59:35","No","No","No","Internal"]
[null,null,null,28077,60423,"30_Fri Dec 02 2022 13:01:02 GMT+0800","2022-11-23T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Crew Messroom  chairs fabric found dirty","","General Appearance","Inappropriate Procedure","","","","","All the Messroom chairs, Recreation Room chairs cleaned properly, and covered with plastics for better protection during docking times.","2023-02-22T23:59:35","","Completed","2023-01-27T23:59:35","No","No","No","Internal"]
[null,null,null,28086,89988,"30_Thu Dec 01 2022 12:29:15 GMT+0800","2022-11-23T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Fenders not kept ready on deck when at Anchor.","Miscellaneous","Mooring","Knowledge Based","","","","","SAME TIME THE FENDERS WERE TAKEN OUT & RIGGED","2022-12-23T23:59:35","","Completed","2022-11-23T23:59:35","No","No","No","Internal"]
[null,null,null,28087,98385,"30_Fri Dec 02 2022 10:20:34 GMT+0800","2022-11-23T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Cleaning of Dust / Rust particles near fish plate.","Miscellaneous","General Appearance","Inappropriate Procedure","11.3","Medium","","","Rust Particles & Dust near fish plate cleaned","2022-12-23T23:59:35","","Completed","2022-11-25T23:59:35","No","No","No","Internal"]
[null,null,null,28088,68531,"30_Fri Dec 02 2022 11:37:14 GMT+0800","2022-11-23T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Renew filter and Oil for Air inlet connection port and stbd Pilot ladder and Gangway.","Deck - Machinery","ISM Related","Equipment Related","5.47","Medium","","","Cleaning/ Inspection/ Renewal of oil for all the Air inlet filters for davits, Cpastain, Gangway, pilot ladder completed.","2022-12-23T23:59:35","","Completed","2022-11-26T23:59:35","No","No","No","Internal"]
[null,null,null,28089,60807,"30_Fri Dec 02 2022 10:25:26 GMT+0800","2022-11-23T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Ship Staff Insp.","Port and STBD Manifold dip tray to be cleaned / clear rust particles","Miscellaneous","General Appearance","Inappropriate Procedure","11.3","Medium","","","Cleaning completed.","2022-12-23T23:59:35","","Completed","2022-11-28T23:59:35","No","No","No","Internal"]
[null,null,null,28091,92286,"30_Fri Dec 02 2022 12:53:30 GMT+0800","2022-11-23T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Personnel Transfer basket Annual testing not carried out","Miscellaneous","ISM Related","Equipment Related","","","","","Annual testing of Personnel transfer basket carried out in June 2022. Next due in June 2023.","2023-02-22T23:59:35","","Completed","2022-11-25T23:59:35","No","No","No","Internal"]
[null,null,null,28092,59618,"30_Fri Dec 02 2022 10:59:25 GMT+0800","2022-11-23T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Renew oil for STBD Pilot Ladder. hoist motor","Deck - Machinery","ISM Related","Equipment Related","5.47","Medium","","","Oil Renewed","2023-02-22T23:59:35","","Completed","2022-11-28T23:59:35","No","No","No","Internal"]
[null,null,null,28093,25543,"30_Fri Dec 02 2022 10:27:44 GMT+0800","2022-11-23T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Port Manifold area cleaning.","Miscellaneous","General Appearance","Inappropriate Procedure","11.3","Medium","","","Port manifold area washed & cleaned","2023-02-22T23:59:35","","Completed","2022-11-25T23:59:35","No","No","No","Internal"]
[null,null,null,28094,89916,"30_Wed Dec 07 2022 21:44:43 GMT+0800","2022-11-23T23:59:35","Defect,Observation","Ship Staff","Ship Staff Insp.","Fresh water Generator Sea water feed line was wasted and leaking.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","All 3 sections of Seawater Feed line fabricated and boxed back.","2023-02-17T23:59:35","","Completed","2022-11-28T23:59:35","No","No","No","Internal"]
[null,null,null,28095,31318,"30_Fri Dec 02 2022 12:12:13 GMT+0800","2022-11-23T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Port side Lifeboat  Fwd coxwain glass is not clear ","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.29","High","","","Renewed  the glass","2023-01-22T23:59:35","","Completed","2022-11-28T23:59:35","No","No","No","Internal"]
[null,null,null,28096,60325,"30_Wed Dec 07 2022 21:37:41 GMT+0800","2022-11-23T23:59:35","Defect,Observation","Ship Staff","Ship Staff Insp.","ME Unit 5 Cylinder cover water leaking from jacket, defective O ring.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","ME unit 5 cylinder cover taken out for jacket o ring replacement, as it was leaking. Jacket dismantled & de rusted , replaced o rings and assembled the jacket. Same time cylinder cover seal ring also changed. Assembled the cylinder cover and engine tried out, found satisfactory.","2023-02-23T23:59:35","","Completed","2022-11-29T23:59:35","No","No","No","Internal"]
[null,null,null,28097,21847,"30_Tue Dec 06 2022 13:56:12 GMT+0800","2022-11-23T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","The COP lower bearing excess grease to be removed asap and correct procedure to be established and train all crew.","Cargo Mach.","Cargo / Ballast Systems","Inappropriate Procedure","","","","","All 3 COP Lower bearing cover removed, excess grease removed & applied new grease.","2022-12-25T23:59:35","","Completed","2022-12-01T23:59:35","No","No","No","Internal"]
[null,null,null,28098,90408,"30_Fri Dec 02 2022 12:33:02 GMT+0800","2022-11-23T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ODME operating procedure to be reviewed and flush the lines so that during decanting ODME operates smoothly.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","All the lines are flushed during monthly calibration.","2023-02-22T23:59:35","","Completed","2022-11-27T23:59:35","No","No","No","Internal"]
[null,null,null,28099,65545,"30_Fri Dec 02 2022 12:48:01 GMT+0800","2022-11-23T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Mooring Winch Break band testing at least 2 tests to be carried out after Joining.","Deck - Mooring Machinery","Mooring","Inappropriate Procedure","9.7","Medium","","","Carried out 2 Winch Brake test","2023-02-22T23:59:35","","Completed","2022-12-03T23:59:35","No","No","No","Internal"]
[null,null,null,28100,65962,"30_Fri Dec 02 2022 12:38:04 GMT+0800","2022-11-23T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","The Mooring winch oil glass found painted at various locations ","Miscellaneous","General Appearance","Inappropriate Procedure","","","","","Oil sighting glass of all the winches cleaned","2023-01-22T23:59:35","","Completed","2022-12-03T23:59:35","No","No","No","Internal"]
[null,null,null,28090,99768,"30_Tue Dec 06 2022 11:34:22 GMT+0800","2022-11-24T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Return oil filter for AFT and FWD Hydraulic system for Deck machinery to renew as its not changed since past one year.","Deck - Mooring Machinery","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Return oil filter for AFT and FWD Hydraulic system for Deck machinery renewed.","2023-02-23T23:59:35","","Completed","2022-11-27T23:59:35","No","No","No","Internal"]
[null,null,null,28079,58825,"30_Wed Dec 07 2022 18:13:52 GMT+0800","2022-11-27T23:59:35","Observation","Ship Staff","Ship Staff Insp.","ER steam 6 k reducer line non return valve is leaking as per indication.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Valve renewed","2023-01-28T23:59:35","","Completed","2023-02-11T23:59:35","No","No","No","Internal"]
[null,null,null,25957,null,"30_Sat Jul 02 2022 04:41:30 GMT+0000","2022-12-02T23:59:35","Defect","Ship Staff","Ship Staff Insp.","IG Pressure Repeater Panel on Bridge Showing error reading.","Inert Gas","Cargo / Ballast Systems","Equipment Related","6.22","Medium","","","New Repeater panel recieved at singapore and installed on place now it is working satisfactory.","2023-06-02T23:59:35","DJAG220148","Completed","2023-06-23T23:59:35","No","No","No","Internal","PO# DJAG220148 issued to maker KASHIWA. Spare delivering at next call SINGAPORE in OCT 2022.\nUnderstood that this defect is sorted in June 2023, which please confirm."]
[null,null,null,28083,69828,"30_Wed Dec 07 2022 22:14:09 GMT+0800","2022-12-02T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Main engine exhaust expansion joint near soot collecting tank found with minor damage. Need to renew at next convenient opportunity.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Bellow renewed in DD","2023-03-02T23:59:35","ME EXHAUST GAS EXPANSION JOINT DJAG220246","Completed","2023-02-17T23:59:35","No","No","No","Internal"]
[null,null,null,28082,85755,"30_Sat Dec 10 2022 12:46:41 GMT+0800","2022-12-05T23:59:35","Defect","Ship Staff","Ship Staff Insp.","VLSFO bunker manifold ( starboard- forward)   isolation valve gear damage","Deck - Pipe / Fittings","MARPOL Related","Equipment Related","6.8","High","","","Valve renewed.","2023-02-05T23:59:35","","Completed","2023-02-07T23:59:35","No","No","No","Internal"]
[null,null,null,28342,68015,"30_Fri Jan 06 2023 09:15:48 GMT+0800","2022-12-20T23:59:35","Defect","Ship Staff","Ship Staff Insp.","3 sectons of VRCS Hydraulic line ( 1 Pressure & 2 return ) found wasted & heavily rusted","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.4","Very High","","","Fabricated & renewed","2023-01-20T23:59:35","","Completed","2023-01-01T23:59:35","No","No","No","Internal"]
[null,null,null,28341,66397,"30_Thu Dec 29 2022 18:47:58 GMT+0800","2022-12-25T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Port side Hawse pipe cover securing Bracket on main deck found wasted","Miscellaneous","General Appearance","Equipment Related","","","","","Fabricated & renewed","2023-03-24T23:59:35","","Completed","2023-02-16T23:59:35","No","No","No","Internal"]
[null,null,null,28343,93363,"30_Wed Jan 04 2023 09:53:16 GMT+0800","2022-12-30T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Aux engine-1 lube oil priming pump motor failure","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Attempts made to save the motor by applying varnish. Insulation is beyond acceptable limit. Spare ordered. Motor renewed on 7th Jan 2023","2023-01-29T23:59:35","DJAG230001","Completed","2023-01-03T23:59:35","No","No","No","Internal"]
[null,null,null,30555,60926,"30_Wed Mar 08 2023 23:29:52 GMT+0800","2023-01-14T23:59:35","Defect","Ship Staff","Ship Staff Insp.","M/E RPM VALUE SHOWED IN CONNING DISPLAY IS ABOUT HALF OF ACTUAL RPM.","Navigation - Others","Navigation","Equipment Related","4.7","High","","","SERVICE ENGINEER BOARDED THE VESSEL AT SINGAPORE. CARRIED OUT RESETTING OF M/E RPM A/D CHANNEL. M/E RPM SHOWING CORRECTLY ON CONNING DISPLAY.","2023-03-27T23:59:35","","Completed","2023-02-27T23:59:35","No","No","No","Internal"]
[null,null,null,28085,28045,"30_Fri Dec 02 2022 12:36:24 GMT+0800","2023-01-24T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Few pipe supports for steam lines are thinned down","Deck - Pipe / Fittings","General Appearance","Equipment Related","","","","","Fabrication & Renewal Completed","2023-04-23T23:59:35","","Completed","2023-03-06T23:59:35","No","No","No","Internal"]
[null,null,null,28071,89466,"30_Fri Dec 02 2022 11:58:32 GMT+0800","2023-01-28T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","The pipe supports on accommodation casing and engine room casing have rust stains","Deck - Pipe / Fittings","General Appearance","Inappropriate Procedure","11.4","Very High","","","Derusting and painting of pipe supports completed.","2023-05-26T23:59:35","","Completed","2023-04-13T23:59:35","No","No","No","Internal"]
[null,null,null,28073,85792,"30_Fri Dec 02 2022 12:05:43 GMT+0800","2023-01-28T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","The door coaming of Paint room, chemical locker are corroded.","Miscellaneous","General Appearance","Inappropriate Procedure","","","","","Fabricated & renewed","2023-03-06T23:59:35","","Completed","2023-02-27T23:59:35","No","No","No","Internal"]
[null,null,null,28074,48092,"30_Fri Dec 02 2022 12:21:11 GMT+0800","2023-01-28T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Few Mooring hydraulic pipelines have corrosion signs","Deck - Mooring Machinery","General Appearance","Equipment Related","11.4","Very High","","","Fabrication & Renewal of corroded section of hydraulic pipes completed.","2023-04-26T23:59:35","","Completed","2023-03-29T23:59:35","No","No","No","Internal"]
[null,null,null,28078,88540,"30_Fri Dec 02 2022 10:48:40 GMT+0800","2023-01-28T23:59:35","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Internet condition of ship very week signal.","Miscellaneous","MLC Related","Equipment Related","","","","","Shore technician attended the vessel on 03 March 2023 at Singapore System health check & hardware / software checks carried out, All found in order. However there is slightest improvement in internet speed. \nInternet speed monitored for one month and found to be satisfactory.","2023-04-26T23:59:35","","Completed","2023-03-28T23:59:35","No","No","No","Internal"]
[null,null,null,28084,56129,"30_Fri Dec 02 2022 11:44:15 GMT+0800","2023-01-28T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Mooring Hydraulic Line on STBD Side boat deck Found with spot Rust.","Deck - Mooring Machinery","General Appearance","Equipment Related","11.4","Very High","","","Derusting & painting Completed","2023-04-26T23:59:35","","Completed","2023-03-10T23:59:35","No","No","No","Internal"]
[null,null,null,30551,44001,"30_Wed Mar 08 2023 20:22:17 GMT+0800","2023-02-04T23:59:35","Defect","Ship Staff","Ship Staff Insp.","STBD Windlass clutch operating lever & STBD windlass  high and low speed operating lever block found leaking","Deck - Mooring Machinery","Mooring","Equipment Related","","","","","Oring Renewed & leak rectified","2023-05-03T23:59:35","","Completed","2023-02-24T23:59:35","No","No","No","Internal"]
[null,null,null,30552,25492,"30_Wed Mar 08 2023 20:25:06 GMT+0800","2023-02-06T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Port side Provision crane Hydraulic valve block found leaking","Deck - Machinery","General Appearance","Equipment Related","","","","","Leak rectified","2023-05-05T23:59:35","","Completed","2023-02-24T23:59:35","No","No","No","Internal"]
[null,null,null,28081,87821,"0_Wed Dec 07 2022 18:19:34 GMT+0800","2023-02-14T23:59:35","Observation","Ship Staff","Ship Staff Insp.","BWTS, TRO unit's main switch is giving loose contact with the operating key","Cargo Mach.,Deck - Machinery","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","No loose contact observed in last 3 operations.","2023-06-26T23:59:35","","Completed","2023-07-12T23:59:35","No","No","No","Internal","Please send email for the same along with attempted repair, we will get Maker's advise in order to assist vessel."]
[null,null,null,30564,67062,"30_Wed Mar 01 2023 18:33:12 GMT+0800","2023-02-21T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Steering gear-2 hydraulic by pass valve & connecting piece threads damaged.","Critical Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","By-pass valve block changed with new spare received.","2023-05-26T23:59:35","DJAG 230066","Completed","2023-04-13T23:59:35","No","No","No","Internal"]
[null,null,null,30559,51949,"30_Wed Mar 08 2023 16:30:11 GMT+0800","2023-02-27T23:59:35","Defect","Ship Staff","Ship Staff Insp.","HFO purifier No.1 is giving bowl leak alarm.","E/R - Purifier","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Purifer 4000hrs routines carried out. All O rings were renewed. \nBowl and disc cleaning carried out. Purifier tried out; working satisfactory and kept stand-by","2023-03-11T23:59:35","","Completed","2023-03-05T23:59:35","No","No","No","Internal"]
[null,null,null,30566,40044,"30_Thu Mar 16 2023 11:51:29 GMT+0800","2023-02-27T23:59:35","Defect","Ship Staff","Ship Staff Insp.","The Controller of the Stbd Provision Crane burnt and needs to be renewed.","Deck - Machinery","General Appearance","Equipment Related","8.50","Medium","","","New controller fixed and crane tried out. \nFound to be working satisfactory.","2023-05-30T23:59:35","DJAG230020","Completed","2023-04-29T23:59:35","No","No","No","Internal"]
[null,null,null,30565,79910,"30_Wed Mar 08 2023 16:24:58 GMT+0800","2023-03-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","pH sensor of Sea water inlet found to be showing incorrect readings.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","New sensor was installed and calibrated. Currently it's showing accurate readings.","2023-04-26T23:59:35","","Completed","2023-04-10T23:59:35","No","No","No","Internal"]
[null,null,null,30560,94857,"30_Thu Mar 09 2023 13:22:49 GMT+0800","2023-03-02T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","Main engine unit no.3 cylinder head stud aft of exhaust bellow found broken.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Broken stud replaced at Suez with old spare. ","2023-03-27T23:59:35","","Completed","2023-03-14T23:59:35","No","No","No","Internal"]
[null,null,null,30563,27520,"30_Sun Mar 12 2023 20:51:47 GMT+0800","2023-03-05T23:59:35","Defect","Ship Staff","Ship Staff Insp.","WMP 002 Sampling pump was observed to have a water ingress in the motor. ","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Pump renewed with new spare received. As of now it 's working satisfactorily.","2023-06-05T23:59:35","","Completed","2023-04-10T23:59:35","No","No","No","Internal"]
[null,null,null,30561,76651,"30_Sat Apr 01 2023 23:01:36 GMT+0800","2023-03-21T23:59:35","Observation","Ship Staff","Ship Staff Insp.","During routine inspection it was noticed that pressure gauge on fire/foam line at stbd side bridge wing is damaged (glycerin leaking from the gauge). Immediately the pressure gauge was replaced with new one.","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.38","High","","","Damaged pressure gauge was immediately renewed with new one. Same tested and found working satisfactory.","2023-04-21T23:59:35","","Completed","2023-03-21T23:59:35","No","No","No","Internal"]
[null,null,null,30535,97676,"30_Wed Mar 29 2023 17:54:37 GMT+0800","2023-03-25T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Control air dryer (membrane type) differential pressure gauge found defective.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Pressure gauge renewed","2023-06-25T23:59:35","DJAG230092","Completed","2023-06-30T23:59:35","No","No","No","Internal","Noted on RO DJAG230092 for control air dryer differential pressure gauge. The same will be supplied to the vessel."]
[null,null,null,30562,91860,"30_Wed Apr 05 2023 02:24:14 GMT+0800","2023-03-30T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Oxygen sensor of one of the RX-517 multi-gas detector (Sr. No. 3Y8060026RN) is malfunctioning. During normal operation it is showing O2 content as 15.8 % and equipment is in continuous alarm mode.  Fresh air and span calibration of the oxygen sensor is also failing. ","Miscellaneous","ISM Related","Equipment Related","5.23","Very High","","","RO raised for oxygen sensor.\nNew gas equipment received on 13 April 2023 at Sabine Lighterage area, USA.","2023-06-11T23:59:35","DJAG235047","Completed","2023-04-10T23:59:35","No","No","No","Internal"]
[null,null,null,30537,82517,"30_Tue Apr 18 2023 03:49:20 GMT+0800","2023-04-01T23:59:35","Observation","Ship Staff","Ship Staff Insp.","No.2 Hydrophore pump motor controller malfunctioning","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","It was observed while running motor was tanking high current than nominal range, it was not tripped on overload, so its main contactor and overload inspected and found contacts inside was totally burned, renewed contactor and overload relay. now pump in use and it is running satisfactory with all parameter in range.","2023-07-01T23:59:35","DJAG230088","Completed","2023-07-08T23:59:35","No","No","No","Internal","Noted on RO DJAG230088, please send email for this defect / rectification as well."]
[null,null,null,30543,11722,"30_Sun Apr 30 2023 22:31:21 GMT+0800","2023-04-08T23:59:35","Defect","Ship Staff","Ship Staff Insp.","1 hotplate out 4 is not operational, hotplate is not heating up  on 4, 5, 6.","Accommodation","General Appearance","Equipment Related","11.16","Low","","","New hotplates recieved, renewed 3 hotplates on place now it is working satisfactory.","2023-07-11T23:59:35","DJAG230070","Completed","2023-06-30T23:59:35","No","No","No","Internal","Noted on RO DJAG230070 for hot plate. will supply soon."]
[null,null,null,30539,42239,"30_Sun Apr 30 2023 22:14:29 GMT+0800","2023-04-20T23:59:35","Defect","Ship Staff","Ship Staff Insp.","COT 5P level not reading, faulty TGE","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.12","Medium","","","Recieved new TGE module and installed on place, now level showing correct, SAAB rada level gauging now working satisfactory.","2023-07-11T23:59:35","DJAG230098","Completed","2023-06-12T23:59:35","No","No","No","Internal","Noted on same, approved for supply, should have been received and fitted.\n\nPlease update as applicable."]
[null,null,null,30542,17987,"30_Wed May 03 2023 21:37:00 GMT+0800","2023-04-29T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Chattering noise observed on main steam valve of Aux boiler #2.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Main steam stop valve renewed, ","2023-07-30T23:59:35","DJAG230102","Completed","2023-07-09T23:59:35","No","No","No","Internal","Noted on RO DJAG230102. we will supply the same soonest."]
[null,null,null,30541,96480,"30_Sat Jun 03 2023 11:25:58 GMT+0800","2023-05-13T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Winch M8 speed found low during heaving and lowering as compared to other winches","Deck - Mooring Machinery","Mooring","Equipment Related","9.14","Medium","","","Oil check carried out ; troubleshooting in progress","2023-07-31T23:59:35","","Completed","2023-08-01T23:59:35","No","No","No","Internal","Vessel changed the auto speed control valve block, problem sorted out."]
[null,null,null,30533,14593,"30_Fri Jun 02 2023 17:44:51 GMT+0800","2023-05-15T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Alarm \"battery fault\" triggered on S band Radar UPS","Navigation - RADAR","Navigation","Equipment Related","4.7","High","","","Recieved new battery( DJAG230115), installed in UPS, now it is working satisfactory. ","2023-08-15T23:59:35","DJAG230115","Completed","2023-06-25T23:59:35","No","No","No","Internal","Noted on DJAG230115, same will be supplied soonest."]
[null,null,null,30534,75673,"30_Tue Mar 28 2023 07:21:42 GMT+0800","2023-06-12T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Meat room Evaporator tray & drain pipe heating element is not functional","Accommodation","MLC Related","Equipment Related","10.32","Very High","","","New heating element installed","2023-09-12T23:59:35","DJAG230078","Completed","2023-09-15T23:59:35","No","No","No","Internal","Noted on RO DJAG230078, same will be supplied to the vessel. at Singapore around 28-Aug-2023"]
[null,null,null,30538,82064,"30_Sun Apr 30 2023 21:57:17 GMT+0800","2023-06-22T23:59:35","Defect","Ship Staff","Ship Staff Insp.","ME FO Circulating pump #2 magnetic coupling sealing cover is found to be leaking.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Magnetic coupling and its cover renewed, tried out , found satisfactory","2023-09-22T23:59:35","DJAG230094","Completed","2023-09-16T23:59:35","No","No","No","Internal","Noted on RO DJAG230094, same will be connected at Singapore"]
[null,null,null,30536,79604,"30_Wed Mar 15 2023 14:47:30 GMT+0800","2023-06-29T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Slop Tank (P) Stripper suction valve Valve position Indicator in Hydraulic room is not working. But Phsically while operating the valve from CCR its actually closing & opening in pumproom","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","9.14","Medium","","","Need to Renew the Valve position indicator( Valve open shut transmitter ).","2024-03-29T23:59:35","DJAG230080 - Hydraulic Valve Remote control System","Completed","2023-12-21T23:59:35","No","No","No","Internal","Noted on RO DJAG230080 to Renew the Valve position indicator. Spares are ready for delivery and AGW, it will be connected to the vessel at Singapore on 28 Aug 2023."]
[null,null,null,28080,74071,"0_Wed Dec 07 2022 18:16:24 GMT+0800","2023-07-11T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Port fresh water tank gauge is not functional","Hull & Tanks","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","PORT FRESH WATER TANK LEVEL GAUGE TO RENEWED.\nV-DJAG049704/23-PORT FRESH WATER TANK LEVEL GAUGE","2023-12-03T23:59:35","DJAG230096","Completed","2023-12-03T23:59:35","No","No","No","Internal",""]
[null,null,null,31393,63843,"0_Sun Aug 27 2023 19:55:26 GMT+0800","2023-07-20T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","\tAir Con for the VFD is to be installed.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.37","Medium","","","All three air con for VFD installed.","2023-10-20T23:59:35","","Completed","2023-09-26T23:59:35","No","No","No","Internal"]
[null,null,null,31395,88772,"0_Sun Aug 27 2023 19:33:31 GMT+0800","2023-07-20T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","\tEGCS – WMS002 pump is broken","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","NEW AIR DRIVEN PUMP INSTALLED","2023-10-20T23:59:35","GC-JAGUAR-002-23 Claim Report Form (WMP 002 Pump failure)","Completed","2023-09-11T23:59:35","No","No","No","Internal"]
[null,null,null,31397,79044,"0_Sun Aug 27 2023 19:49:27 GMT+0800","2023-07-20T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","\tWet garbage locker has water ingress","Deck - Pipe / Fittings","General Appearance","External Factors","11.12","Low","","","Line blown through and tested","2023-09-15T23:59:35","","Completed","2023-09-15T23:59:35","No","No","No","Internal"]
[null,null,null,31398,26590,"0_Sun Aug 27 2023 19:17:43 GMT+0800","2023-07-20T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","\tMooring Winch M7 – slow for first few seconds upon starting ","Deck - Mooring Machinery","Mooring","Equipment Related","9.14","Medium","","","vessel tried out mooring winch M7 , found  working satisfactory","2023-10-20T23:59:35","","Completed","2023-08-01T23:59:35","No","No","No","Internal"]
[null,null,null,31401,71296,"30_Sun Aug 27 2023 18:59:49 GMT+0800","2023-07-20T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","\tCargo Oil tank 5S– pressure sensor showing sensor fail","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.13","Medium","","","sensor  renewed","2023-10-20T23:59:35","","Completed","2023-07-31T23:59:35","No","No","No","Internal"]
[null,null,null,31399,15454,"0_Sun Aug 27 2023 19:59:05 GMT+0800","2023-07-31T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Aft hydraulic system cooler sea water pipe is leaking","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","pipe removed and  welding repair carried out.","2023-10-31T23:59:35","","Completed","2023-08-02T23:59:35","No","No","No","Internal"]
[null,null,null,31400,49648,"0_Sun Aug 27 2023 20:02:55 GMT+0800","2023-08-04T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Deck seal water pressure gauge line valve found leaking","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","valve renewed","2023-11-04T23:59:35","","Completed","2023-08-06T23:59:35","No","No","No","Internal"]
[null,null,null,33352,75596,"30_Mon Sep 25 2023 18:24:04 GMT+0800","2023-08-07T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","Accomodation air con #1 tripped in high suction gas temerature","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","All three cylinder opened up, found stage three suction plate is broken, same renewed, all stages suction and discharge valves inspected, air con tried out , found satisfactory.","2023-11-04T23:59:35","","Completed","2023-08-10T23:59:35","No","No","No","Internal"]
[null,null,null,33351,23280,"0_Mon Sep 25 2023 18:30:38 GMT+0800","2023-08-11T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","Accomodation air con #2 tripped due to high suction gas temerature","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","All three stage cylinder opened up, found stage #2 suction valve in broken condition , suction valve plate renewed, all three stages suction valves, discharge valves and unloading mechanisms inspected, air con tried out, found satisfactory","2023-11-04T23:59:35","","Completed","2023-08-14T23:59:35","No","No","No","Internal"]
[null,null,null,33350,35133,"0_Mon Sep 25 2023 18:45:23 GMT+0800","2023-08-23T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Hose handling crane #2 personnel and main hoisting limit switches is not working","Deck - Machinery","Cargo / Ballast Systems","Equipment Related","8.50","Medium","","","Hose handling crane #2 both personnal and main hoisting limit switch cam and screw arrangement opened up, found bearings damaged, same renewed, tried out, found satisfactory.","2023-11-20T23:59:35","","Completed","2023-08-26T23:59:35","No","No","No","Internal"]
[null,null,null,33358,54228,"30_Mon Sep 25 2023 20:35:46 GMT+0800","2023-09-06T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Ejector pump discharge  valve is leaking","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Ejector pump discharge valve renewed, tried out and found satisfactory.","2023-12-05T23:59:35","","Completed","2023-09-08T23:59:35","No","No","No","Internal"]
[null,null,null,33362,74485,"0_Mon Sep 25 2023 20:40:32 GMT+0800","2023-09-16T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Sea water seepage from EGCS sea water  pump #2 discharge line welding ","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","sea water discharge pipe replaced with spare one.","2023-12-15T23:59:35","","Completed","2023-09-18T23:59:35","No","No","No","Internal"]
[null,null,null,33363,69159,"30_Thu Sep 28 2023 15:46:04 GMT+0800","2023-09-22T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Elevator - car door inverter error","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.37","Medium","","","Annual servicing by shore technician and all componenents checked  .Elevator working in good order.","2023-12-20T23:59:35","DJAG235083","Completed","2023-11-29T23:59:35","No","No","No","Internal"]
[null,null,null,33361,64996,"30_Mon Oct 23 2023 13:46:49 GMT+0800","2023-10-09T23:59:35","Defect","Ship Staff","Ship Staff Insp.","ME jacket water preheater is leaking","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","ME jacket pre heater opened up, gaskets renewed","2024-01-08T23:59:35","","Completed","2023-10-11T23:59:35","No","No","No","Internal"]
[null,null,null,33353,63594,"0_Fri Nov 17 2023 09:45:00 GMT+0800","2023-10-30T23:59:35","Defect","Ship Staff","Ship Staff Insp.","AE #1 jacket water preheater thermostat is not working","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","V-DJAG049806/23-//AE1 THERMOSTAT WITH SENSOR//AE1 THERMOSTAT WITH SENSOR FOR PRE HEATER MALFUNCTIONING SAME RENEWED.","2024-01-30T23:59:35","DJAG230211","Completed","2023-12-12T23:59:35","No","No","No","Internal"]
[null,null,null,33336,14766,"30_Thu Nov 16 2023 19:20:55 GMT+0800","2023-11-16T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Removable Stanchion near port and starboard gangway sheared off from base due to wastage","Deck - Pipe / Fittings","General Appearance","External Factors","11.3","Medium","","","Hot work needs to be carried out in ER workshop.","2024-02-15T23:59:35","","Completed",null,"No","No","No","Internal"]
[null,null,null,33354,96778,"30_Fri Dec 15 2023 17:47:45 GMT+0800","2023-11-29T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","cow line pressure Guage not working","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.34","High","","","COW line pressure guage renewed","2024-02-29T23:59:35","","Completed","2023-12-15T23:59:35","No","No","No","Internal","Noted that COW line pressure guage has been renewed."]
[null,null,null,33355,40438,"30_Fri Dec 15 2023 17:52:17 GMT+0800","2023-11-29T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","pressure guage on fire line not working","LSA / FFA","Safety / LSA / FFA","Equipment Related","8.69","Medium","","","Fire line pressure gauge renewed","2024-02-29T23:59:35","","Completed","2023-12-15T23:59:35","No","No","No","Internal","Noted that Fire line pressure gauge is renewed.\nThe defect is closed."]
[null,null,null,33357,49799,"30_Tue Dec 12 2023 20:31:18 GMT+0800","2023-11-29T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Main engine both hydraulic electric start up pump spider coupling is consumed and need to be renewed.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related,External Factors,Industry Issue","10.32","Very High","","","Spider Coupling  renewed. and job has been updated in unplanned job in PMS.","2024-02-29T23:59:35","","Completed","2023-12-27T23:59:35","No","No","No","Internal","Noted as completed and closed.\nNoted job has been updated in unplanned job in PMS."]
[null,null,null,33344,72986,"30_Sun Dec 31 2023 18:56:17 GMT+0800","2023-12-11T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Port side windlass operating platform railing broken ","Deck - Pipe / Fittings","General Appearance","External Factors","11.3","Medium","","","To be repaired by using Cold work","2024-02-29T23:59:35","","Completed",null,"No","No","No","Internal"]
[null,null,null,33343,30660,"30_Tue Dec 12 2023 21:17:39 GMT+0800","2023-12-15T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Main engine JCW controller is malfunctioning for inlet jacket temperature.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related,External Factors,Human Error,Industry Issue,Inappropriate Procedure","10.32","Very High","","","The positioner was replaced and calibrated.  Presently the controller is working from AMS. ","2024-03-15T23:59:35","","Completed","2024-05-10T23:59:35","No","No","No","Internal","Continue email communication is order to pin point the faulty component. "]
[null,null,null,33348,64091,"0_Mon Sep 25 2023 21:06:50 GMT+0800","2023-12-15T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Galley hot plate power switch is not functional","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.37","Medium","","","Hot plate power switch to be renewed, requisition raised.","2024-03-15T23:59:35","DJAG230178","Completed","2024-03-08T23:59:35","No","No","No","Internal","Noted on RO DJAG230178, the same will be supplied  to the vessel soonest possible."]
[null,null,null,33338,21720,"30_Tue Dec 12 2023 20:57:29 GMT+0800","2023-12-18T23:59:35","Defect,Observation","Ship Staff","Ship Staff Insp.","Pressure Calibration hand pump is malfunctioning for operation, vessel has lost (-1 to 60 bar pressure calibration gauge)","Miscellaneous","Eng. / Strg. Comp.","Equipment Related,Human Error,Industry Issue","10.32","Very High","","","Pump quotation has been approved and will receive spare pressure calibration pump in next suitable port. Pressure calibrator received at Singapore on 23.may.2024","2024-03-18T23:59:35","","Completed","2024-05-23T23:59:35","No","No","No","Internal","Do advise RO number for follow up."]
[null,null,null,33360,18079,"30_Sun Dec 31 2023 18:50:31 GMT+0800","2023-12-20T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Port side life boat engine exhaust flap found broken ","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.30","High","","","New flap to be fabricated and replaced.","2023-12-21T23:59:35","","Completed","2023-12-21T23:59:35","No","No","No","Internal"]
[null,null,null,34091,11563,"30_Tue Jan 30 2024 07:10:33 GMT+0800","2023-12-22T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Provision Crane 10 T port side Main Control Valve slewing handle oil seal is leaking.","Deck - Machinery","Eng. / Strg. Comp.","Equipment Related,Human Error,External Factors","8.50","Medium","","","Vessel has dismantled the operating lever and tried to rectify with spare seal but we observed the seal shaft face are in corroded condition and operating handle still slightly leaking for oil.temporarily repaired has been carried out. spares received","2024-03-22T23:59:35","DJAG240037","Completed","2024-05-27T23:59:35","No","No","No","Internal"]
[null,null,null,33334,83488,"0_Fri Nov 17 2023 09:39:01 GMT+0800","2023-12-22T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Incinerator garbage feeding sluice feeding door solenoid valve is not working.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Solenoid valve need to be renewed, requisition raised ( DJAG230212 ).\nAt present make shift arrangement has been fitted for air cylinder.","2024-03-22T23:59:35","DJAG230212","Completed","2024-03-08T23:59:35","No","No","No","Internal","DJAG230212 will be supplied to the vessel soonest.\n\nNoted temporary arrangement has been made for the Air Cylinder."]
[null,null,null,33335,25054,"30_Sun Dec 03 2023 09:20:41 GMT+0800","2023-12-22T23:59:35","Defect","Ship Staff","Ship Staff Insp.","ME HFO MASS FLOW METER NOT WORKING","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related,Inappropriate Procedure,Industry Issue","10.32","Very High","","","ME MASS FLOW METER ELECTRONIC PCB IS IN BURNT CONDITION AND TO BE REPLACED WITH NEW ONE,SERVICE ENGINEER HAS ATTENDED THE VESSEL IN SINGAPORE ON 29.11.2023.","2024-03-22T23:59:35","DJAG235114 &DJAG240016","Completed","2024-03-07T23:59:35","No","No","No","Internal","The same is ready for delivery and will be connected at Long Beach on around 07-Mar-2024."]
[null,null,null,33345,51106,"30_Sun Dec 31 2023 18:59:27 GMT+0800","2023-12-25T23:59:35","Defect,Observation","Ship Staff","Ship Staff Insp.","Main Engine Fuel oil backwash Filter oil is leaking from gland of changeover cock.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related,External Factors,Inappropriate Procedure","10.32","Very High","","","All in line O-ring/seal rings to be renewed.","2024-03-25T23:59:35","","Completed","2023-12-29T23:59:35","No","No","No","Internal"]
[null,null,null,33359,95475,"30_Sun Dec 31 2023 19:02:07 GMT+0800","2023-12-26T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","Anemometer rotary cup on main mast broken. due to which Anemometer was showing wrong reading.","Navigation - Others","Navigation","Equipment Related","4.7","High","","","Anemometer Rotary Cup replaced with the spare cup on board. ","2024-03-26T23:59:35","","Completed","2023-12-27T23:59:35","No","No","No","Internal"]
[null,null,null,33356,36481,"30_Sun Dec 31 2023 18:56:58 GMT+0800","2023-12-27T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Stern tube #2 pump coupling spider to be renewed.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related,External Factors,Industry Issue","10.32","Very High","","","Vessel staff renewed the spider and coupling,same job has been updated in PMS as a unplanned.","2024-03-27T23:59:35","","Completed",null,"No","No","No","Internal"]
[null,null,null,34094,86494,"30_Fri Jan 12 2024 16:23:04 GMT+0800","2024-01-04T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Ballast valve no BA014 WBT No 3P Stripper Suction valve not operating from remote CCR panel.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.11","Medium","","","suspected solenoid valve in forward bosun store block not giving enough open pressure. air purging carried out.","2024-03-04T23:59:35","","Completed","2024-01-13T23:59:35","No","No","No","Internal"]
[null,null,null,34093,98380,"30_Tue Jan 16 2024 23:37:07 GMT+0800","2024-01-15T23:59:35","Observation,Defect,Non Conformity","Ship Staff","Ship Staff Insp.","HOSPITAL & ENGINE ROOM 2ND DECK FIRE DETECTION SYSTEM MANUAL CALL POINT MALFUNCTIONING.","Critical Equip.","Safety / LSA / FFA","Equipment Related,External Factors,Inappropriate Procedure","10.32","Very High","","","AT PRESENT MANUAL CALL POINT HAS BEEN BY PASSED WITH CORRECT POLARITY AND FIRE DETECTION SYSTEM IS NORMAL FOR ALL OTHER ALARMS.SPECIFIC MANUAL CALL POINT TO BE RENEWED.","2024-04-16T23:59:35","DJAG240070","Completed","2024-03-14T23:59:35","No","No","No","Internal","MCP is send to Long Beach. the same will be connected to the vessel on 28-Feb."]
[null,null,null,34089,43447,"30_Mon Jan 22 2024 00:22:30 GMT+0800","2024-01-16T23:59:35","Critical Equipment,Defect,Observation,Non Conformity","Ship Staff","Ship Staff Insp.","Topping up compressor was out of order due to 1st stage bearing failure.","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related,External Factors,Inappropriate Procedure","10.32","Very High","","","Compressor is completely dismantled and renewed all bearings except 1st stage and 2nd stage con rod bearing is due for unavailable of spares.","2024-04-16T23:59:35","DJAG240072","Completed","2024-03-13T23:59:35","No","No","No","Internal","Spares are send to Long Beach, same will be connected to the vessel on 07-Mar-2024"]
[null,null,null,34092,73156,"30_Mon Jan 22 2024 00:19:07 GMT+0800","2024-01-20T23:59:35","Defect,Observation","Ship Staff","Ship Staff Insp.","Incinerator Secondary burner diesel oil pump is leaking from pump cover.","E/R - Pumps,E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related,External Factors,Human Error,Inappropriate Procedure","10.32","Very High","","","Vessel has dismantled the pump cover and noticed a previously the pump cover was assembled with cold work putty due to hairline crack on cover. tried to repair again but not found satisfactory. Need to be renewed cover of the pump.Temporarily leak has been contained by cold work. New pump was received and replaced. Pump tested for operation. working satisfactorily.   ","2024-04-20T23:59:35","DJAG240083","Completed","2024-05-28T23:59:35","No","No","No","Internal","RO DJAG240083 noted, same will be supplied soonest."]
[null,null,null,33339,86032,"30_Tue Dec 12 2023 21:09:52 GMT+0800","2024-02-16T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Control air refrigerant dryer is malfunctioning","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related,External Factors,Human Error,Industry Issue","10.32","Very High","","","Vessel suspecting thermostatic expansion valve is not functioning and valve to be renewed. Power switch renewed and tested for operation. Working satisfactorily. ","2024-05-16T23:59:35","DJAG240067 & DJAG240063","Completed","2024-04-14T23:59:35","No","No","No","Internal","Noted on RO DJAG240067 & DJAG240063. \nwe will supply the spares first, vessel to try to resolve the issue with spares, if the same is not by spares, we will consider supplying complete refrigerant dryer.\n\nETO has successfully sorted out this issue."]
[null,null,null,33342,34609,"30_Tue Dec 12 2023 20:36:50 GMT+0800","2024-03-18T23:59:35","Defect,Observation","Ship Staff","Ship Staff Insp.","Deck seal both pump strainer casing observed in corroded condition and inlet 2 pcs,5K40 valve is not holding for water.","Inert Gas,Cargo Mach.","Eng. / Strg. Comp.","Equipment Related,External Factors,Industry Issue","10.32","Very High","","","Strainer body and valves to be renewed. Temporarily cold work has been carried out. Filter body received and replaced. Satisfactory. ","2024-06-18T23:59:35","DJAG230233 & DJAG240015","Completed","2024-05-31T23:59:35","No","No","No","Internal","DJAG230233 & DJAG240015 - noted on these two RO - we will supply the same soonest. \nPlease check/ confirm if same was supplied in May 2024 in Zhoushan?"]
[null,null,null,33346,44703,"30_Thu Dec 07 2023 11:05:17 GMT+0800","2024-03-18T23:59:35","Defect","Ship Staff","Ship Staff Insp.","PROVISION COMPRESSOR #1 BOTH SHAFT BUSH WORN OUT CONDITION AND SHAFT SEAL IS LEAKING DUE TO HIGH RADIAL CLEARANCE.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related,External Factors,Industry Issue","10.32","Very High","","","SPARE COMPRESSOR RECEIVED, INSTALLED AND TESTED FOR OPERATION. WORKING SATISFACTORILY. ","2024-06-18T23:59:35","DJAG240009 & DJAG240010","Completed","2024-06-16T23:59:35","No","No","No","Internal","Note on RO DJAG240009 & DJAG240010, we will supply the same once ready.\nNew Compressor is supplied to the vessel on 24-May-2024"]
[null,null,null,37067,97981,"30_Sun Aug 18 2024 22:45:52 GMT+0800","2024-03-22T23:59:35","Defect","Ship Staff","Ship Staff Insp.","AE performance Diesel doctor DK-20 is malfunctioning.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Off landed for repair. Awaiting return of equipment from maker after repair. Received and tested during performance measurement. Satisfactory. ","2024-08-15T23:59:35","","Completed","2024-07-22T23:59:35","No","No","No","Internal"]
[null,null,null,37068,82885,"30_Sun Aug 18 2024 22:43:08 GMT+0800","2024-03-22T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Hose handling crane port system hydraulic oil filter body observed slightly in rusted condition.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.50","Medium","","","Complete filter body to be renewed. spares received, to be replaced during this voyage.  Filter renewed. ","2024-07-31T23:59:35","DJAG240055","Completed","2024-07-03T23:59:35","No","No","No","Internal"]
[null,null,null,34088,32959,"30_Tue Jan 30 2024 07:19:10 GMT+0800","2024-04-01T23:59:35","Observation,Defect","Ship Staff","Ship Staff Insp.","Ballast Water Treatment Plant (BWTS) Gas Separator sampling water Husky welden type pump malfunctioning.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related,External Factors,Industry Issue","6.22","Medium","","","Vessel has dismantled the Husky welden type pump and check all components for any damage marks, but visually found satisfactory. Still Pump is malfunctioning.at present drain valve has been installed and will order same capacity welden pump in stores. Pump received at Singapore on 23 May 2024. New pump has been installed and tested for operation. Working satisfactorily.  ","2024-07-01T23:59:35","DJAG240099","Completed","2024-06-05T23:59:35","No","No","No","Internal","New pump supplied and pls install same."]
[null,null,null,35408,37835,"30_Wed May 29 2024 11:06:44 GMT+0800","2024-04-06T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Aux boiler chemical dosing pump found not working. Found ball bearings broken and electric motor low insulation.","E/R - Aux. Mach.,E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","New pump received and installed. Tested for operation. Satisfactory. ","2024-07-05T23:59:35","DJAG240137","Completed","2024-05-30T23:59:35","No","No","No","Internal","noted and pls update"]
[null,null,null,35405,97118,"30_Wed May 29 2024 11:13:05 GMT+0800","2024-04-15T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Steering gear No.1 pump coupling gear teeth are found worn. To be replaced.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Vessel has one set of gears spare. To be replaced at next convenient opportunity. Pump and motor coupling renewed. Assembled in order and tested for operation. Working satisfactorily. ","2024-07-04T23:59:35","","Completed","2024-06-15T23:59:35","No","No","No","Internal","noted."]
[null,null,null,35410,24950,"30_Wed May 29 2024 10:33:54 GMT+0800","2024-05-03T23:59:35","Defect","Ship Staff","Ship Staff Insp.","EGCS SW pumps 1&2 discharge pipe elbows are found leaking. To be removed and to be repaired in engine room workshop. ","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","EGCS SW pumps 1&2 discharge pipe elbows were removed and inspected in engine room workshop. There was localized pitting at some placed and weld joint eroded from inside of pipe. Both elbows were removed and repaired by welding.  ","2024-05-15T23:59:35","","Completed","2024-05-12T23:59:35","No","No","No","Internal"]
[null,null,null,35411,19938,"30_Wed May 29 2024 10:18:48 GMT+0800","2024-05-13T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Main engine JCFW system leaks were detected at JCFW pumps. It was noted that the valves were not holding when attempted to isolate the system for leak rectification. ","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Valves received. JCFW/LT CFW system was drained after black out. Valves were replaced. Angle check valve 5K200, 5K50 SDNR Globe valve,  Angle check valve 10K65, Butterfly valves 5K200,  ","2024-05-20T23:59:35","","Completed","2024-05-16T23:59:35","No","No","No","Internal"]
[null,null,null,36425,91094,"0_Fri Jun 14 2024 22:05:11 GMT+0800","2024-05-25T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","EGCS Sea water pump # 3 Suction pipe elbow before the suction valve is leaking.","E/R - Pipes/ valves & fittings,E/R - Main Engine,E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related,Industry Issue","10.32","Very High","","","Pipe was removed and repaired by welding in engine room workshop. Pressure tested in engine room workshop at 7 bar by water pressure. No leak. Pipe fitted back and the pump was put into service. Satisfactory.","2024-08-25T23:59:35","","Completed","2024-07-05T23:59:35","No","No","No","Internal","Noted that pipe has been repaired on 04-July. Please close this defect in DDRL."]
[null,null,null,36426,53478,"30_Fri Jun 14 2024 21:55:21 GMT+0800","2024-05-25T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Main Engine LO Hydraulic filter actuator does not move the filter.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Hydraulic actuator overhaul carried out. working satisfactorily. The defect is being closed.","2024-08-25T23:59:35","","Completed","2024-07-30T23:59:35","No","No","No","Internal","If actuator is working correctly, this defect can be closed in DDRL. please revert.\nNoted that Hydraulic actuator overhaul carried out and now working satisfactorily."]
[null,null,null,35404,19063,"30_Wed May 29 2024 11:55:39 GMT+0800","2024-05-25T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","HFO purifier No.2 transducer not responding alarm triggers often.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Transducer cable was replaced but alarm still kept triggering. Further it was established that the sealing water was not supplied to purifier due to NR valve found fitted in reverse direction. The block was removed and assembled correctly. The transducer is functioning normal.","2024-08-25T23:59:35","","Completed","2024-07-11T23:59:35","No","No","No","Internal","Noted and will arrange spares asap. PO issued to Alfa Laval.\nNoted as completed and closed"]
[null,null,null,36429,81466,"30_Fri Jun 14 2024 22:25:32 GMT+0800","2024-05-25T23:59:35","Defect,Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Starboard mooring Windlass hydraulic oil leaking from operating lever.","Deck - Mooring Machinery","Mooring","Equipment Related","10.32","Very High","","","Operating lever shaft sealing ring and seals renewed.  Stbd windlass tried out, no leaks observed.","2024-08-25T23:59:35","","Completed","2024-06-06T23:59:35","No","No","No","Internal","Noted as Operating lever shaft sealing ring and seals renewed. Completed and closed."]
[null,null,null,35403,96901,"30_Wed May 29 2024 10:58:01 GMT+0800","2024-06-16T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Forward deck mach. hyd. power unit PLC is found defective.","Deck - Machinery,Deck - Mooring Machinery","Mooring","Equipment Related","9.14","Medium","","","PLC renewed with spares received. programmed as per instructed. system working satisfactory.","2024-09-16T23:59:35","DJAG240163","Completed","2024-08-30T23:59:35","No","No","No","Internal","The spares has been ordered to Eyde Mooring Solution.   If fwd power is required more vsl can interchange with Aft .. \nThis one is ready for delivery."]
[null,null,null,33333,84847,"30_Fri Nov 17 2023 09:29:57 GMT+0800","2024-06-29T23:59:35","Defect","Ship Staff","Ship Staff Insp.","CCR CCTV is not working","Miscellaneous","General Appearance","Equipment Related","7.12","High","","","CCR CCTV: Camera is still non-operational. New camera was checked by connecting to 8-port POE converter (converter supplied by maker). Still the new camera IP address is not appearing on NVR screen. As communicated earlier, there is no IP address ladled on new camera. Since no IP address known and not appearing by connecting to POE converter, we can`t proceed further. Awaiting advise from office. ..... \n CCR camera started working after renewing the LAN cable( Connected in wrong sequence at both ends) and re-installing it in the system.","2024-09-29T23:59:35","DJAG240179","Completed","2024-12-28T23:59:35","No","No","No","Internal","Please update once spares are installed.\nPlease confirm spares is received at Singapore on 04-July?"]
[null,null,null,35407,44806,"30_Wed May 29 2024 11:35:38 GMT+0800","2024-06-30T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Vessel experienced high differential pressure across M/E Maotti LO back wash filter. When we tried to isolate the filter, it was noted that the valves are not holding.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","ME LO auto backwash filter inlet valve renewed. ","2024-09-30T23:59:35","DJAG240039\nDJAG240170","Completed","2024-11-27T23:59:35","No","No","No","Internal","Valve seat has been supplied to the vessel. To repair same before load port."]
[null,null,null,36428,67917,"30_Mon Jun 17 2024 13:55:00 GMT+0800","2024-07-10T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Aux engine # 2 unit # 3 exhaust gas temperature sensor is broken inside cylinder head pocket.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Cylinder head renewed with spare overhauled cylinder head.","2024-10-10T23:59:35","DJAG240068, DJAG240223","Completed","2025-03-15T23:59:35","No","No","No","Internal",""]
[null,null,null,37066,95957,"30_Thu Jul 25 2024 21:49:54 GMT+0800","2024-07-10T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Garbage locker exhaust fan was not rotating with power on and tripping by overload.   ","Elect. Mach. & Equip.","Safety / LSA / FFA","External Factors,Human Error","6.20","Medium","","","On dismantling found fan blades were stuck with housing due to spray paint sucked inside. Suspect the paint entered due to spay paint in garbage locker. Garbage locker exhaust fan motor overhauled. Motor winding measured 200Mohms initially, insulation spray applied on winding. motor both DE and NDE bearing changed with new. Fan blade cleaned and balancing checked in workshop.\nmotor terminal box found fully rusted and hole inside, new box fabricated and fixed. After boxed up motor winding IR measured more than 1000Mohms, fan installed and tried out working good in order. V-DJAG026119/20","2024-07-17T23:59:35","","Completed","2024-07-14T23:59:35","No","No","No","Internal"]
[null,null,null,37318,30642,"30_Sat Aug 24 2024 11:41:59 GMT+0800","2024-07-12T23:59:35","Defect","Ship Staff","Ship Staff Insp.","During the Routine testing of Aux boiler no: 01, Observed that after the purging cycle gets completed, started panting  prior firing, later on once the minimum firing load achieved, boiler become stable.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","SETTINGS IN MAIN BOILER PANEL Q501 CHANGED AS PER MAKER'S INSTRUCTIONS. BOILER TRIED OUT. ALL SATISFACTORY.","2024-10-12T23:59:35","","Completed","2024-10-01T23:59:35","No","No","No","Internal","Communication with Maker of Aux Boiler ( MHI) is on. Keep replying to teh queries raised by them to sort this out."]
[null,null,null,37063,12479,"30_Sun Aug 18 2024 22:50:56 GMT+0800","2024-07-18T23:59:35","Critical Equipment","Ship Staff","Ship Staff Insp.","Topping up/emergency air compressor cooling water pump is found stuck, shaft not rotating and electric motor giving 440V low insulation alarm.","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Pump and motor dismantled and parts inspected. Electric motor winding found burnt. renewed with new spares received on board.","2024-10-18T23:59:35","DJAG240158","Completed","2024-10-26T23:59:35","No","No","Yes","Internal","Noted on RO DJAG240158, same will be supplied soon."]
[null,null,null,37062,43836,"30_Sat Aug 17 2024 04:20:37 GMT+0800","2024-07-19T23:59:35","Defect","Ship Staff","Ship Staff Insp.","EGCS Water monitoring system (WMS)-002 gives sample low flow alarm.","E/R - Main Engine","ISM Related","Equipment Related","10.32","Very High","","","Husky diaphragm pump driving air solenoid valve is found defective. Presently the solenoid is removed and air supply is given directly. The pump has to be stopped manually after stopping EGCS and need to start pump manually before start EGCS. SPARES Renewed and made system operational.","2024-10-19T23:59:35","DJAG240150-EGCS WMS 002 SAMPLE PUMP SOLENOID VALVE AND FITTING","Completed","2024-10-31T23:59:35","No","No","Yes","Internal","Please check the RO number. This RO is ordered to Alfa Laval. This is for different spares."]
[null,null,null,37307,45045,"30_Sat Aug 24 2024 02:23:23 GMT+0800","2024-08-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Cargo & bunker Tank overfill alarm air horn hooter damaged on deck.","Cargo Mach.,Elect. Mach. & Equip.","Cargo / Ballast Systems","Equipment Related","8.14","Very High","","","Air horn fitting checked, the hooter found broken condition, Alarm tried out working satisfactory.\nAir horn replaced with spares received.\n","2024-11-01T23:59:35","","Completed","2024-11-04T23:59:35","No","No","No","Internal"]
[null,null,null,37308,93243,"30_Sat Aug 24 2024 02:29:00 GMT+0800","2024-08-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","BWTS H2 blower pressure transmitter not working","Elect. Mach. & Equip.","Cargo / Ballast Systems","Equipment Related","2.13","Low","","","Pressure transmitter renewed, working satisfactory","2024-11-01T23:59:35","RO DJAG240113","Completed","2025-01-17T23:59:35","No","No","No","Internal","Noted on RO DJAG240113. Same will be supplied at First Opportunity."]
[null,null,null,37320,56614,"30_Sat Aug 24 2024 09:19:30 GMT+0800","2024-08-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","HFO purifier no: 01 was overhauled in Feb 2024, As per the report, same has been boxed back with all the seal rings except one Guide ring, as the Guide ring was not available onboard. Same has been Order under RO DJAG240217","E/R - Purifier","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","HFO Purifier no: 01, opened up, Missing Guide ring added to the bowl, Other Parts inspected,  Purifier tried out, found working satisfactory.","2024-09-10T23:59:35","DJAG240217","Completed","2024-08-30T23:59:35","No","No","No","Internal"]
[null,null,null,37064,91709,"30_Sun Aug 18 2024 22:33:02 GMT+0800","2024-08-15T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Air conditioning plant #2 compressor unit main controller running hrs reading to be displayed in negative reading, & 2nd stage unloader rocker arm locking pin found in damaged condition.","E/R - Aux. Mach.","","Equipment Related","10.32","Very High","","","1.  Running hour meter is working on AMS. ACS controller display is showing negative sign. \n2. Compressor 2nd stage was giving abnormal sound, 2nd stage dismantled and inspected. Piston pin and piston have scoring marks. The small end bush found loose inside connecting rod and bush too much worn. \n3. Renewed piston and connecting rod assembly. \n4. 2ND stage all four rocker arms renewed. \n5. Oil filter changed, Suction oil filter cleaned  and sump oil renewed. \nRunning test carried out, satisfactory.   ","2024-11-15T23:59:35","DJAG230175","Completed","2024-08-22T23:59:35","No","No","Yes","Internal","Noted on RO DJAG230175. This is year 2023 RO, which is closed due to year end. Please make RO in 2024 and advise RO Number."]
[null,null,null,37065,22707,"30_Sun Aug 18 2024 22:37:19 GMT+0800","2024-08-15T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Sewage treatment plant oh radical lamp is not working.","E/R - Aux. Mach.","","","10.32","Very High","","","OH Radical lamp fitted in place. ","2024-11-15T23:59:35","DJAG240018","Completed","2024-09-10T23:59:35","No","No","No","Internal","DJAG240018 is ordered to RUSH enterprise, and is ready for delivery."]
[null,null,null,37319,77587,"30_Sat Aug 24 2024 02:52:16 GMT+0800","2024-08-23T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Main engine platform fire/general alarm solenoid malfunctioning.","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.35","Medium","","","solenoid coil voltage checked, found solenoid defective, also mild crack on hooter. same spare alarm fitting renewed. working satisfactory.","2024-08-31T23:59:35","","Completed","2024-08-23T23:59:35","No","No","No","Internal"]
[null,null,null,37311,71249,"30_Sun Sep 15 2024 15:59:11 GMT+0800","2024-08-26T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Main Engine unit no:3  slight leakage from the accumulator base O-ring  observed,","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","ME unit 3 accumulator removed, Base O-rings renewed. 1 no plug renewed. System tried out, no leaks observed.","2024-11-05T23:59:35","DJAG240227","Completed","2024-11-22T23:59:35","No","No","No","Internal","Please refer to the email send from vessel DHT Puma to be sure that location of the leak is correctly identified,"]
[null,null,null,37310,59935,"30_Sun Sep 15 2024 16:58:16 GMT+0800","2024-08-29T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Main Engine Hydraulic actuator unit #5 & Unit #6:: Slight Oil leaking from base.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Main Engine Hydraulic actuator unit #5 & Unit #6 all bolts retightened. No leaks observed. ","2024-11-05T23:59:35","","Completed","2024-11-22T23:59:35","No","No","No","Internal","Noted on same. Do check on the  forwarded email from sister vessel DHT Puma on the importance of locating the leak correctly."]
[null,null,null,37315,95331,"30_Sun Sep 15 2024 16:08:46 GMT+0800","2024-08-29T23:59:35","Defect","Ship Staff","Ship Staff Insp.","EGCS WMS 02, Communication error alarm is triggered, RS-485 Convertor is malfunctioning.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.11","Medium","","","New convertor configured, fitted and tried-out, working satisfactory","2025-02-20T23:59:35","DJAG240228","Completed","2025-02-19T23:59:35","No","No","No","Internal","RO DJAG240228 is noted, same will be processed soonest possible."]
[null,null,null,37312,92534,"30_Sat Aug 31 2024 03:07:25 GMT+0800","2024-08-30T23:59:35","Defect","Ship Staff","Ship Staff Insp.","220V low insulation is perpetual.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","investigation for all 220V system individually needs to be carried out and fault to identify and rectify the same. : Investigation done , a number of fittings, equipment have been made up . Insulation issue is under control now. ","2024-11-30T23:59:35","","Completed","2024-12-01T23:59:35","No","No","No","Internal","Please update progress to sort this 220V low insulation for ever. \nDo report the same in a separate email to auto electric department if any shore help is required."]
[null,null,null,37321,45165,"30_Sat Aug 31 2024 03:23:10 GMT+0800","2024-08-30T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Steering gear mushroom vent drain pipe corroded/wasted.","Hull & Tanks","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","New Pipe fabricated & Installed.","2024-11-30T23:59:35","","Completed","2024-09-03T23:59:35","No","No","No","Internal"]
[null,null,null,38812,82308,"30_Wed Sep 25 2024 13:25:43 GMT+0800","2024-09-03T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Alternator no-1 (R-WINDING) Temperature found showing erratic  temperature value, which was triggering the alarm: HIGH TEMPERATURE OF R-WINDING.  Same value was hunting from normal value to 200 ° C.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Alternator no-1 (R-WINDING) Temperature found showing erratic , spare sensor (already installed in the winding by maker) put in  use by interchanging  the connection, connection made tested ,found R-S-T winding showing corrected temperature value as of now.","2024-10-05T23:59:35","","Completed","2024-09-04T23:59:35","No","No","No","Internal"]
[null,null,null,38799,44495,"30_Mon Sep 23 2024 13:04:04 GMT+0800","2024-09-09T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Observed the small leakage on the Galley drain line section connecting to the ER port side Strom Valve, Temporary repair carried out.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Line replaced with pre-fabricated one.","2024-11-10T23:59:35","","Completed","2024-11-05T23:59:35","No","No","No","Internal"]
[null,null,null,37314,92114,"30_Sun Sep 15 2024 19:45:50 GMT+0800","2024-09-12T23:59:35","Defect","Ship Staff","Ship Staff Insp.","IG Scrubber Pump Suction valve is not holding, By closing the valve, still the Suction pressure is sustain. Unable to drain out the water from pump casing.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","2.16","Medium","","","Travel for suction valve increased by few mm. now the valve is shut and holding good. Anodes renewed. ","2024-12-12T23:59:35","DJAG240231","Completed","2024-11-05T23:59:35","No","No","No","Internal","Noted on RO DJAG240231, same will be supplied at Singapore during ballast voyage."]
[null,null,null,37309,41044,"30_Sun Sep 15 2024 16:42:15 GMT+0800","2024-09-13T23:59:35","Defect","Ship Staff","Ship Staff Insp.","ANEMOMETER AT 130 antenna unit wind speed fan is not rotating.","Navigation - Others","Navigation","Equipment Related","4.3","Medium","","","Anemometer fitted with new spare received. Working satisfactorily.","2024-12-13T23:59:35","DJAG245094","Completed","2024-10-25T23:59:35","No","No","No","Internal","Order for spare has been placed as per DJAG245094."]
[null,null,null,38792,99546,"30_Mon Sep 30 2024 12:06:59 GMT+0800","2024-09-16T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Stern Tube LO pump no:02, was leaking from Mechanical seal.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Stern Tube LO Pump no :02, was leaking from seal, same opened up for overhauling, Pump Driving & Driven gear cleaning & Inspection carried out, Found in order, Mechanical seal renewed along with the new Oil seal. On opening of pump, found the Coupling for both motor & pump side was fabricated before, Same renewed . Pump boxed back, Tried out, found working satisfactory, Ampere drawn by the pump found with in the required limit.","2024-10-10T23:59:35","","Completed","2024-09-18T23:59:35","No","No","No","Internal"]
[null,null,null,38793,90340,"30_Mon Sep 30 2024 12:02:09 GMT+0800","2024-09-16T23:59:35","Defect","Ship Staff","Ship Staff Insp.","During the ER Pumps loop changeover , ME Fuel Oil Supply pump no: 01,  found no building up pressure, also abnormal sound was detected.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Pump opened up for overhauling, parts inspection done, Driving & Driven screw inspected, found satisfactory. Bearing renewed, Magnetic coupling found in good state. Pump Boxed back. Tried out, found slight increase in pressure. No abnormal sound observed. RV opened up, found the seat & sliding face was damaged, same replaced, pump started, tried out, found working satisfactory. Ampere drawn by the pump was within the limit.","2024-10-10T23:59:35","","Completed","2024-09-25T23:59:35","No","No","No","Internal"]
[null,null,null,38796,74278,"30_Wed Sep 25 2024 13:34:12 GMT+0800","2024-09-16T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Observed the Sewage Treatment Plant, OH-Radical lamp is not working, ","Elect. Mach. & Equip.","MARPOL Related","Equipment Related","10.32","Very High","","","OH Radical lamp replaced, Lamp BALLAST unit supply voltage checked, found BALLAST is malfunctioning & Out voltage observed 0Volt. Same has been ordered for new Electronic BALLAST. Moreover for all ports we are collecting the sewage in tanks for complete port stay; sealing the tank outlet.\n\n\nBallast renewed with new received spares.","2024-10-31T23:59:35","DJAG240234","Completed","2024-10-29T23:59:35","No","No","No","Internal"]
[null,null,null,38800,57638,"30_Mon Sep 30 2024 11:55:02 GMT+0800","2024-09-16T23:59:35","Defect","Ship Staff","Ship Staff Insp.","HFO Purifier no: 02,  Fuel oil heater found leaking from steam side flange.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","HFO Heater isolated, Fuel & Steam valves closed, heater end cover removed, gasket renewed, heater tubes cleaning done, Steam leakage rectified.","2024-10-15T23:59:35","","Completed","2024-09-23T23:59:35","No","No","No","Internal"]
[null,null,null,38804,55756,"30_Mon Sep 23 2024 13:01:04 GMT+0800","2024-09-17T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Deck seal Low flow alarm triggering, as the suction line is partially chocked, Common suction line valve is not holding, moreover, suction line two sections are wasted from small portion.  Entire line is connected to the sea chest without any isolation.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Suction line removed and a new valve was installed. A section of pipe line is renewed after the valve. Line is clear now, pump discharge pressure is increased from 2 bar to 4 bars. ","2024-11-20T23:59:35","","Completed","2024-11-16T23:59:35","No","No","No","Internal"]
[null,null,null,38813,72571,"30_Mon Sep 30 2024 11:51:26 GMT+0800","2024-09-18T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Main Engine Jacket water heater leaking from flange.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Heater isolated, Jacket water & steam lines valve closed,  Heater flanges gasket renewed, Leakage rectified.","2024-10-15T23:59:35","","Completed","2024-09-25T23:59:35","No","No","No","Internal"]
[null,null,null,38798,52261,"30_Thu Oct 24 2024 15:36:52 GMT+0800","2024-09-20T23:59:35","Defect","Ship Staff","Ship Staff Insp.","PA System Mic in the electrical room is malfunctioning. ","Miscellaneous","Communication","Equipment Related","8.102","Low","","","Mic fitted with new received spares.","2024-12-20T23:59:35","DJAG240235","Completed","2024-10-29T23:59:35","No","No","No","Internal"]
[null,null,null,38794,76117,"30_Fri Sep 27 2024 15:37:05 GMT+0800","2024-09-26T23:59:35","Observation","Ship Staff","Ship Staff Insp.","MCP 001 COMMUNICATION FAULT GENERATED ON EGCS HMI.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.11","Medium","","","REBOOTING THE SYSTEM RESET ALARM","2024-10-27T23:59:35","","Completed","2024-10-19T23:59:35","No","No","No","Internal"]
[null,null,null,38811,20670,"30_Fri Sep 27 2024 15:50:04 GMT+0800","2024-09-27T23:59:35","Defect","Ship Staff","Ship Staff Insp.","BWTS Main  ( flow control valve)  FCV 1211 IS NON-OPERATIONAL. ","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","6.21","High","","","New positioner installed, calibrated and tried-out, working satisfactory","2024-12-27T23:59:35","","Completed","2025-02-07T23:59:35","No","No","No","Internal"]
[null,null,null,38797,69398,"30_Sat Oct 26 2024 19:37:42 GMT+0800","2024-10-25T23:59:35","Observation","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","01 unit of navigation light (upper main mast) was found fused at the time of testing. As per the deck logbook records, testing of the navigation light was carried out every watch and noted in good order.","Navigation - Others,Navigation - GMDSS & Communication","Navigation","Equipment Related","4.2","Medium","","","Fused light bulb was replaced immediately upon departure from the port and was both upper and lower lights were found working satisfactory.","2025-01-24T23:59:35","N/A","Completed","2024-10-25T23:59:35","No","No","No","External"]
[null,null,null,38795,87669,"30_Fri Oct 11 2024 11:38:01 GMT+0800","2024-11-09T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Inspection to be carried out in Ship's Laundry / Dryer room for any hanging boiler suits / combustible material which may have the potential to create unsafe condition due to rolling / falling over heater element.","Accommodation,Miscellaneous,Elect. Mach. & Equip.","Safety / LSA / FFA","Human Error","11.14","Medium","","","Ship's Laundry spaces are checked on daily / regular basis during Fire Rounds as per procedure. Weekly verification of the spaces is being carried out Master / Ch Off. during the accommodation rounds. As per the requirements, the area is verified additionally to ensure that no combustible material is in near vicinity of the heating element.  All crew were briefed with regards to the procedures and to comply strictly with the same. Lint filter for the Dryer machines shall be opened / cleaned prior every usage by the user.","2025-02-09T23:59:35","N/A","Completed","2024-10-15T23:59:35","No","No","No","Internal","Noted as completed and closed."]
[null,null,null,38801,66114,"30_Tue Nov 05 2024 09:31:11 GMT+0800","2024-11-09T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","OIL SEAL FOR DG#2 PRIMING LO PUMP LEAKY.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","OIL SEAL TO BE RENEWED WITH SPARES ON BOARD. / Shaft dismantled, found marks on shaft ( shaft was built up some time ago), same polished on lathe and fitted back with same oil seal. Test run carried out. No leak is present.","2024-12-09T23:59:35","","Completed","2024-11-18T23:59:35","No","No","No","Internal","Noted as completed and closed."]
[null,null,null,38802,94401,"30_Fri Oct 11 2024 09:37:20 GMT+0800","2024-11-09T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","series interface relay ABB-RBR121A-24 V ac/dc, MALFUNCTIONING.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","INTERFACE RELAY RENEWED, PURIFIER WORKING SATISFACTORY.","2025-02-09T23:59:35","DJAG240274","Completed","2024-11-14T23:59:35","No","No","No","Internal","Noted as completed and closed."]
[null,null,null,38803,97978,"30_Mon Sep 30 2024 11:38:51 GMT+0800","2024-11-09T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","EGCS Sea water pump no: 03, suction pipe was leaking, same was removed & section welded with the insert, leakage rectified.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.23","Medium","","","New pipe section fabricated and replaced with old repaired pipe. System tried out, no leaks observed.","2024-12-09T23:59:35","","Completed","2024-11-21T23:59:35","No","No","No","Internal","Noted as completed and closed."]
[null,null,null,38805,77145,"30_Sat Oct 05 2024 15:23:05 GMT+0800","2024-11-09T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Forward bosun store stbd bilge well high level alarm float defective.","Hull & Tanks","Structural Condn. / WT integrity ","Equipment Related","8.61","Medium","","","Forward bosun store stbd bilge well high level alarm float renewed. Tried out working satisfactory.","2025-02-09T23:59:35","DJAG240255","Completed","2025-01-07T23:59:35","No","No","No","Internal","Noted as completed and closed"]
[null,null,null,38806,81334,"30_Sat Oct 05 2024 23:59:42 GMT+0800","2024-11-09T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","LSHFO sett. tank pump auto cut out switch found malfunctioning, getting activated after starting pump even when tank level is low in actual","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.8","Medium","","","Present switch was removed, repaired, fitted back the same and tried-out, working satisfactory.","2025-02-09T23:59:35","DJAG240255","Completed","2025-01-22T23:59:35","No","No","No","Internal","Noted as completed and closed."]
[null,null,null,38807,81843,"30_Wed Oct 23 2024 09:42:04 GMT+0800","2024-11-09T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Neutralization injection pump no.2 FAILURE alarm triggered on BWTS Monitor.\nUpon investigation found digital display for the pump unit non-operational (Switched Off)\nFuses (3-AMP) checked and found blown off. Same renewed but to no result.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","6.21","High","","","Aft peak neutralizing unit pump renewed. Tried out working satisfactory.","2025-02-09T23:59:35","DJAG240285","Completed","2025-01-06T23:59:35","No","No","No","Internal","Noted as completed and closed."]
[null,null,null,38810,81426,"30_Sat Oct 19 2024 14:19:20 GMT+0800","2024-11-09T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","FIRE WIRE REEL GEAR BOX OIL SEAL LEAKING.","Deck - Machinery","Safety / LSA / FFA","Equipment Related","5.4","High","","","FWD FIRE WIRE GEAR BOX SHAFT CLEANED. NEW LUBRICATING OIL FILLED UP TO THE CORRECT LEVEL. GEAR OIL FILLING CAP RENEWED. TRIED OUT THE MOTOR, WORKING STISFACTORY, NO LEAKAGES.","2025-02-09T23:59:35","DJAG240282","Completed","2024-11-25T23:59:35","No","No","No","Internal","Noted as completed and closed"]
[null,null,null,37305,97740,"30_Sat Aug 24 2024 02:36:54 GMT+0800","2024-11-09T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","M/E L.O cooler temperature controller is not working","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","controller needs replacement. Controller repairs carried out. Pneumatic valve block of positioner replaced form an old used controller. All components function verified. Zero setting re-adjusted. Controller is working now.","2025-02-09T23:59:35","DJAG240288","Completed","2024-12-07T23:59:35","No","No","No","Internal","Noted as completed and closed."]
[null,null,null,39809,61992,"30_Sat Mar 15 2025 15:02:16 GMT+0800","2024-11-19T23:59:35","Critical Equipment","Ship Staff","Nav Audit / Verification","Doppler Log - When Vessel Speed over ground less than 2.0 kts.; the doppler becomes unreliable and provides inaccurate readings.","Navigation - Echo Sounder / Speed Log","","","4.7","High","","","Deferred to DD, defect added in REFMAN.","2025-05-15T23:59:35","","Completed","2025-03-19T23:59:35","No","No","No","Internal","To be checked during 2nd special survey docking. Include the defect in DD Specification in Refmen and close the same."]
[null,null,null,38809,81961,"30_Fri Jan 31 2025 13:23:56 GMT+0800","2024-12-01T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Alarm in MSB \"Emergency Stop source fail\" due to faulty timer contacts, needed to be renewed","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","As vessel got spare timers when renewal of ESB, same was used for renewing the faulty timer, no alarm, system working satisfactory","2025-02-28T23:59:35","","Completed","2025-01-30T23:59:35","No","No","No","Internal"]
[null,null,null,38784,51881,"30_Mon Jan 13 2025 14:29:01 GMT+0800","2024-12-20T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Sewage treatment plant OH radical lamp electronic ballast not working.","Elect. Mach. & Equip.,E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Sewage treatment plant OH radical lamp electronic ballast renewed.","2025-03-05T23:59:35","DJAG250023","Completed","2025-03-05T23:59:35","No","No","No","Internal"]
[null,null,null,38808,58285,"30_Mon Dec 30 2024 08:04:07 GMT+0800","2024-12-28T23:59:35","Other","Ship Staff","Suptd. Insp.","Various relays on Emergency switch board to renew as part of precautionary maintenance. ","Critical Equip.","Emgcy. Systems","Equipment Related","10.32","Very High","","","All the components are renewed and auto function checked, system working satisfactory","2025-02-28T23:59:35","","Completed","2025-01-25T23:59:35","No","No","No","Internal"]
[null,null,null,39812,26713,"30_Sun Mar 16 2025 20:32:25 GMT+0800","2025-01-25T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Main LO filter outlet valve found to be not holding.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Main LO filter outlet valve renewed on 01 APR 2025. New installed v/v that has been used was repaired onboard with new seat ring and seals. ","2025-04-25T23:59:35","","Completed","2025-04-01T23:59:35","No","No","No","Internal","Noted the vessel has 1 spare outlet valve for main LO filter. Plan for renewal at first oppurtunity."]
[null,null,null,39839,67169,"30_Wed Mar 19 2025 16:23:26 GMT+0800","2025-02-26T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","4S P/V valve mesh corroded, to be renewed.","Hull & Tanks","Cargo / Ballast Systems","Equipment Related","","","","","4S P/V valve mesh renewed.","2025-03-25T23:59:35","","Completed","2025-03-03T23:59:35","No","No","No","Internal"]
[null,null,null,39840,92854,"30_Wed Mar 19 2025 16:26:37 GMT+0800","2025-02-26T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Housekeeping / cleaning to be carried out in BWTS Room. Loose items to be secured","Miscellaneous","General Appearance","Behaviour Based","","","","","Housekeeping / cleaning carried out in BWTS Room. All Loose items secured.","2025-03-25T23:59:35","","Completed","2025-03-13T23:59:35","No","No","No","Internal"]
[null,null,null,39841,56277,"30_Wed Mar 19 2025 16:32:31 GMT+0800","2025-02-26T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Load Cell shore calibration to be carried out","Miscellaneous","Mooring","Equipment Related","","","","","Shore Calibrated Load Cell received at Singapore.","2025-05-25T23:59:35","","Completed","2025-02-26T23:59:35","No","No","No","Internal"]
[null,null,null,39842,58740,"30_Wed Mar 19 2025 16:20:05 GMT+0800","2025-02-26T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","2P HFO Tank Vent to derust, Paint & restencil.","Miscellaneous","General Appearance","Equipment Related","","","","","2P HFO Tank Vent derusting and painting completed. Restenciling carried out.","2025-03-25T23:59:35","","Completed","2025-03-18T23:59:35","No","No","No","Internal"]
[null,null,null,39843,26855,"30_Wed Mar 19 2025 16:43:08 GMT+0800","2025-02-26T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","M/E # 3 & #4 unit cylinder head bursting disc safety cap protection cover direction observed to be opening on fuel p/p side of the engine, it should be turned to exhaust side of the engine for safety reasons.","E/R - Main Engine","Eng. / Strg. Comp.","Human Error","10.32","Very High","","","M/E #3 & #4 unit cylinder head bursting disc safety valve protection cover turned in correct direction (opening towards exhaust valve side, so that in case of opening of safety valve person standing on the fuel pump side is safe). Same discussed with all engine room staff regarding the importance of it.","2025-02-28T23:59:35","","Completed",null,"No","No","No","Internal"]
[null,null,null,39844,91093,"30_Wed Mar 19 2025 16:16:04 GMT+0800","2025-02-26T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Mid ship store port side house-keeping and cleaning of bulkheads to carry out.","Miscellaneous","General Appearance","Behaviour Based","","","","","Mid ship store port side house-keeping and cleaning of bulkheads carried out.","2025-04-25T23:59:35","","Completed","2025-03-04T23:59:35","No","No","No","Internal"]
[null,null,null,39845,74568,"30_Wed Mar 19 2025 16:30:15 GMT+0800","2025-02-26T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Sounding cap for sludge collecting tank was found not properly closed, sounding caps to be closed properly after taking sounding of tanks","Miscellaneous","General Appearance","Human Error","10.26","High","","","Sounding caps closed properly and all E/R staff briefed about the importance of closing the sounding caps properly.","2025-02-28T23:59:35","","Completed","2025-02-28T23:59:35","No","No","No","Internal"]
[null,null,null,40273,12535,"30_Tue Mar 25 2025 01:16:19 GMT+0800","2025-03-22T23:59:35","Critical Equipment","Ship Staff","Ship Staff Insp.","Emergency generator radiator found leaking during testing of the Emergency generator","Critical Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Emergency generator Radiator renewed with spare.","2025-03-24T23:59:35","DJAG215044","Completed","2025-03-24T23:59:35","No","No","No","Internal"]
[null,null,null,null,87428,"30_Wed Mar 19 2025 16:35:24 GMT+0800","2025-02-26T08:00:00","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","5 ppm cell for OWS and clean bilge is expiring on 9th March 2025, new calibrated cell to be supplied onboard.","Critical Equip.","MARPOL Related","Equipment Related","6.17","Very High","","","1 New calibrated oil content meter received and installed on OWS. OWS tested, 3 way valve operation checked and alarm tested, all found working satisfactory. New defect created for clean bilge oil content meter renewal.","2025-05-15T08:00:00","DJAG250079","Completed","2025-05-05T08:00:00","No","No","No","Internal","As vessel Singapore call was cancelled, the OCM could not be calibrated. \nNew OCM is ordered to Maker. once the new OCM is available, we will connected the same to vessel."]
[null,null,null,null,62803,"30_Mon Feb 03 2025 20:16:29 GMT+0800","2025-03-03T08:00:00","Other","Ship Staff","Ship Staff Insp.","VECS oxygen sensor needed to be renewed as per PMS, no spare onboard","Deck - Machinery","Cargo / Ballast Systems","Equipment Related","2.12","Low","","","Oxygen sensor not able to calibrate/ not working.  PO raised awaiting for spare","2025-06-30T08:00:00","DJAG250059","Completed","2025-06-19T08:00:00","No","No","No","Internal","Quote has been received for DJAG250059. The same is being reviewed for suitability."]
[null,null,null,null,27898,"30_Wed May 14 2025 08:59:25 GMT+0800","2025-05-06T08:00:00","Defect","Ship Staff","Ship Staff Insp.","IGS deck seal tank low level alarm switch malfunctioning.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","10.35","Very High","","","Requisition DJAG250180 raised. Awaiting for spares.","2025-06-30T08:00:00","DJAG250180","Completed","2025-06-19T08:00:00","No","No","No","Internal"]
[null,null,null,null,83811,"30_Mon Jun 17 2024 13:46:59 GMT+0800","2025-03-28T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Minor oil leak is observed from steering gear #1 hydraulic pump shaft seal.","Navigation - Others","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Both steering gear pumps and motor were overhauled by technicians in Dry dock 2025. Both pumps tested but no leaks observed.","2025-06-28T08:00:00","DJAG240222","Completed","2025-06-18T08:00:00","No","No","Yes","Internal","Noted of RO DJAG240222. The same will be supplied soon.\n\nTo be done in Changhong Shipyard during this Special Survey in around end of May 2025"]
[null,null,null,null,44159,"30_Mon Jun 17 2024 13:49:33 GMT+0800","2025-03-30T08:00:00","Defect,Observation","Ship Staff","Ship Staff Insp.","Minor oil leak is observed from steering gear # 2 hydraulic pump shaft seal.","Navigation - Others","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Both steering gear pumps and motor were overhauled by technicians in Dry dock 2025. Both pumps tested but no leaks observed.","2025-06-29T08:00:00","DJAG240222","Completed","2025-06-18T08:00:00","No","No","Yes","Internal","Noted on RO DJAG240222. same will be supplied soon."]
[null,null,null,null,18553,"30_Wed May 14 2025 08:49:01 GMT+0800","2025-05-04T08:00:00","Observation","Ship Staff","Ship Staff Insp.","DG LO purifier heater steam inlet valve found to be leaking (steam passing even with the valve closed).","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Valve renewed in Dry dock 2025. ","2025-06-15T08:00:00","DJAG250172","Completed","2025-06-18T08:00:00","No","No","No","Internal"]
[null,null,null,null,70664,"30_Tue May 13 2025 11:45:47 GMT+0800","2025-02-26T08:00:00","Observation,Non Conformity","Ship Staff","Ship Staff Insp.","5 ppm cell for clean bilge tank expiring on 9th March 2025, new calibrated cell to be supplied onboard.","Critical Equip.","MARPOL Related","Equipment Related","6.17","Very High","","","Oil content meter renewed. 15 ppm alarm tested and 3 way valve tried out, all found working satisfactory.","2025-06-15T08:00:00","DJAG250079","Completed","2025-06-25T08:00:00","No","No","No","Internal"]
[null,null,null,null,74120,"30_Wed May 14 2025 13:47:39 GMT+0800","2025-05-12T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Main LO purifier 3 way valve found leaking during de sludge cycle. Same needs to be overhauled or renewed.","E/R - Purifier","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Main LO purifier 3 way valve renewed. Purifier tested, all found working satisfactory.","2025-06-30T08:00:00","DJAG250166","Completed","2025-06-18T08:00:00","No","No","No","Internal"]
[null,null,null,null,20564,"0_Tue Nov 26 2024 19:56:04 GMT+0800","2024-11-19T08:00:00","Observation","Ship Staff","Nav Audit / Verification","Steering Gear : There is a discrepancy of 1 to 1.5 deg. between Ordered Rudder angle (Steering Wheel) and actual rudder Angle. Same\nto be rectified.","E/R - Aux. Mach.,Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.39","High","","","Technician attended the job in Dry dock 2025 and has rectified the discrepancy.","2025-07-15T08:00:00","","Completed","2025-06-18T08:00:00","No","No","No","Internal","Please update on investigation and enter the same in DD if cannot be attended while vessel is in service.\n\nTo be done in Changhong Shipyard during this Special Survey in around end of May 2025"]
[null,null,null,null,26056,"30_Tue Nov 26 2024 19:49:09 GMT+0800","2024-11-19T08:00:00","Critical Equipment","Ship Staff","Nav Audit / Verification","Echo Sounder Fwd & Aft transducer displayed depth has substantial and variable discrepancy (0.5m to over 2 mtrs. after allowing for\ntrim correction).","Navigation - Echo Sounder / Speed Log","Navigation","Equipment Related","4.7","High","","","Investigation in progress","2025-06-15T08:00:00","","Completed","2025-06-20T08:00:00","No","No","No","Internal","Please update on investigation and enter the same in DD if cannot be attended while vessel is in service.\n\nTo be done in Changhong Shipyard during this Special Survey in around end of May 2025"]
[null,null,null,null,56975,"30_Wed May 14 2025 09:21:41 GMT+0800","2025-05-06T08:00:00","Breakdown","Ship Staff","Ship Staff Insp.","ECR camera 1 is not operational due to faulty camera. ","Elect. Mach. & Equip.","General Appearance","Equipment Related","","","","","Requisition DJAG250179 raised. Awaiting spares.","2025-06-30T08:00:00","DJAG250179","Completed","2025-06-28T08:00:00","No","No","No","Internal"]
[null,null,null,null,61610,"30_Thu Jun 26 2025 23:27:17 GMT+0800","2025-06-20T08:00:00","Defect","Ship Staff","Ship Staff Insp.","FW Generator overboard valve orientation fitted wrongly by yard ","E/R - Purifier","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Orientation need to be rectified ","2025-09-20T08:00:00","","Completed","2025-06-28T08:00:00","No","No","No","Internal"]
[null,null,null,null,38208,"30_Sat Aug 24 2024 02:44:29 GMT+0800","2025-02-15T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Pump room steam ballast pump water discharge pneumatic transmitter gauge is not working.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","6.22","Medium","","","Normal gauge is fitted and tried not working. Need to be installed new pressure transmitter.","2025-07-30T08:00:00","DJAG240211","Completed","2025-06-19T08:00:00","No","No","No","Internal","RO DJAG240211. noted and is being worked on."]

{"sheet":"Calc","index":2,"n_rows":28,"n_cols":12,"rows_kept":28,"cut":false,"hidden":true,"merged":[]}
["Def_type","Def_cause","Equipments","VIQrefno","Observer_code"]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,"Dim itemSele As Long"]
[null,null,null,null,null,null,null,null,null,null,null,"   dim startRow as integer"]
[null,null,null,null,null,null,null,null,null,null,null,"   startRow=1"]
[null,null,null,null,null,null,null,null,null,null,null,"        For itemSele = 0 To ListBox1.ListCount - 1"]
[null,null,null,null,null,null,null,null,null,null,null,"        If ListBox1.Selected(itemSele) = True Then"]
[null,null,null,null,null,null,null,null,null,null,null,"        Worksheets(\"WorksheetName\").Range(\"A\" & startRow).Value = ListBox1.List(itemSele)"]
[null,null,null,null,null,null,null,null,null,null,null,"        startRow = startRow + 1"]
[null,null,null,null,null,null,null,null,null,null,null,"        End If"]
[null,null,null,null,null,null,null,null,null,null,null,"        Next"]
[null,null,null,null,null,null,null,null,null,null,null,"Dim LastRowA As String"]
[null,null,null,null,null,null,null,null,null,null,null,"        Dim itemSele As Long"]
[null,null,null,null,null,null,null,null,null,null,null,"       Dim startRow as integer"]
[null,null,null,null,null,null,null,null,null,null,null,"        LastRowA = ActiveSheet.Cells(Rows.count, \"A\").End(xlUp).row"]
[null,null,null,null,null,null,null,null,null,null,null,"        startQue = 0"]
[null,null,null,null,null,null,null,null,null,null,null,"        For itemSele = 0 To ListBox1.ListCount - 1"]
[null,null,null,null,null,null,null,null,null,null,null,"        For startRow = 1 To LastRowA"]
[null,null,null,null,null,null,null,null,null,null,null,"        If Worksheets(\"WorksheetName\").Range(\"A\" & startRow).Value = ListBox1.List(itemSele) Then"]
[null,null,null,null,null,null,null,null,null,null,null,"        ListBox1.Selected(itemSele) = True"]
[null,null,null,null,null,null,null,null,null,null,null,"        Exit For"]
[null,null,null,null,null,null,null,null,null,null,null,"        End If"]
[null,null,null,null,null,null,null,null,null,null,null,"        Next j"]
[null,null,null,null,null,null,null,null,null,null,null,"        Next"]
[null,null,null,null,null,null,null,null,null,null,null,"        End If"]

{"sheet":"Areaofobs","index":3,"n_rows":17,"n_cols":2,"rows_kept":17,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Cargo / Ballast Systems",11]
["Cert. & Docu.",2]
["Communication",6]
["Crew Management",3]
["Emgcy. Systems",13]
["Eng. / Strg. Comp.",14]
["General Appearance",15]
["Ice Opns.",17]
["ISM Related",7]
["ISPS Related",10]
["MARPOL Related",9]
["MLC Related",4]
["Mooring",12]
["Navigation",5]
["Safety / LSA / FFA",8]
["Structural Condn. / WT integrity ",16]

{"sheet":"Vessel_type","index":4,"n_rows":1,"n_cols":2,"rows_kept":1,"cut":false,"hidden":true,"merged":[]}
["Vessel_type","ID"]

{"sheet":"Deficiency_type","index":5,"n_rows":8,"n_cols":3,"rows_kept":8,"cut":false,"hidden":true,"merged":[]}
["TITLE","Type of deficiency_description","ID"]
["Breakdown",null,6]
["Critical Equipment",null,4]
["Defect",null,1]
["Guarantee Claim",null,8]
["Non Conformity",null,2]
["Observation",null,3]
["Other",null,7]

{"sheet":"VIQrefno","index":6,"n_rows":427,"n_cols":3,"rows_kept":427,"cut":false,"hidden":true,"merged":[]}
["VIQ_ref_no","Risk Value of observation","ID"]
["1.1","Low",8243]
["1.10","Low",8252]
["1.11","Low",8253]
["1.12","Low",8254]
["1.13","Low",8255]
["1.14","Low",8256]
["1.15","Low",8257]
["1.16","Low",8259]
["1.17","Low",8260]
["1.18","Low",8261]
["1.19","Low",8262]
["1.2","Low",8244]
["1.20","Low",8263]
["1.21","Low",8265]
["1.22","Low",8266]
["1.23","Low",8267]
["1.24","Low",8268]
["1.25","Low",8269]
["1.26","Low",8270]
["1.3","Low",8245]
["1.4","Low",8246]
["1.5","Low",8247]
["1.6","Low",8248]
["1.7","Low",8249]
["1.8","Low",8250]
["1.9","Low",8251]
["1.99","High",11258]
["10.1","Medium",8461]
["10.10","High",8470]
["10.11","Medium",8471]
["10.12","Very High",8472]
["10.13","Very High",8473]
["10.14","Medium",8474]
["10.15","Low",8475]
["10.16","Very High",8476]
["10.17","Very High",8477]
["10.18","High",8478]
["10.19","Very High",8479]
["10.2","Low",8462]
["10.20","High",8480]
["10.21","Medium",8481]
["10.22","Low",8482]
["10.23","Medium",8483]
["10.24","Low",8484]
["10.25","Very High",8485]
["10.26","High",8486]
["10.27","Medium",8487]
["10.28","Low",8488]
["10.29","Medium",8489]
["10.3","Medium",8463]
["10.30","High",8490]
["10.31","Very High",8491]
["10.32","Very High",8492]
["10.33","High",8493]
["10.34","High",8494]
["10.35","Very High",8495]
["10.36","Very High",8496]
["10.37","Medium",8497]
["10.38","Medium",8498]
["10.39","High",8499]
["10.4","High",8464]
["10.40","Medium",8500]
["10.41","Medium",8501]
["10.42","Medium",8502]
["10.43","Medium",8503]
["10.44","Medium",8504]
["10.45","Very High",8505]
["10.46","High",8506]
["10.47","Medium",8507]
["10.48","High",8508]
["10.49","Medium",8509]
["10.5","Low",8465]
["10.50","High",8510]
["10.51","Low",8511]
["10.52","Medium",8512]
["10.53","Medium",8513]
["10.54","High",8514]
["10.55","Low",8515]
["10.6","Very High",8466]
["10.7","Medium",8467]
["10.8","Medium",8468]
["10.9","Medium",8469]
["10.99","High",8516]
["11.1","High",8420]
["11.10","Medium",8429]
["11.11","Very High",8430]
["11.12","Low",8431]
["11.13","Low",8432]
["11.14","Medium",8433]
["11.15","Low",8434]
["11.16","Low",8435]
["11.17","Low",8436]
["11.2","Medium",8421]
["11.3","Medium",8422]
["11.4","Very High",8423]
["11.5","Medium",8424]
["11.6","Medium",8425]
["11.7","High",8426]
["11.8","Low",8427]
["11.9","Low",8428]
["11.99","High",8437]
["12.1","High",8438]
["12.10","High",8448]
["12.11","High",8449]
["12.12","High",8450]
["12.13","High",8451]
["12.14","High",8452]
["12.15","High",8453]
["12.16","High",8454]
["12.17","High",8455]
["12.18","High",8456]
["12.19","High",8457]
["12.2","High",8439]
["12.20","High",8458]
["12.21","High",8459]
["12.3","High",8441]
["12.4","High",8442]
["12.5","High",8443]
["12.6","High",8444]
["12.7","High",8445]
["12.8","High",8446]
["12.9","High",8447]
["12.99","High",8460]
["2.1","Very High",8296]
["2.1.9","Very High",11259]
["2.10","Medium",8304]
["2.11","Medium",8305]
["2.12","Low",8306]
["2.13","Low",8307]
["2.14","Low",8308]
["2.15","Low",8309]
["2.16","Medium",8310]
["2.2","Medium",8297]
["2.3","High",8295]
["2.4","Medium",8298]
["2.5","Medium",8299]
["2.6","Low",8300]
["2.7","High",8301]
["2.8","High",8302]
["2.9","Medium",8303]
["2.99","High",8311]
["3.1","High",8312]
["3.2","Very High",8313]
["3.3","High",8314]
["3.4","Low",8294]
["3.5","Medium",8315]
["3.6","High",8316]
["3.7","Very High",8317]
["3.8","Very High",8318]
["3.99","High",8319]
["4.1","High",8320]
["4.10","High",8329]
["4.11","Medium",8330]
["4.12","Very High",8331]
["4.13","Very High",8332]
["4.14","Very High",8333]
["4.15","Very High",8334]
["4.16","Very High",8335]
["4.17","Very High",8336]
["4.18","Very High",8337]
["4.19","Low",8338]
["4.2","Medium",8321]
["4.20","Very High",8339]
["4.21","High",8340]
["4.22","Low",8341]
["4.23","High",8342]
["4.24","High",8343]
["4.25","Low",8344]
["4.26","Low",8345]
["4.27","High",8346]
["4.3","Medium",8322]
["4.4","High",8323]
["4.5","Very High",8324]
["4.6","Medium",8325]
["4.7","High",8326]
["4.8","Medium",8327]
["4.9","Medium",8328]
["4.99","High",8347]
["5.1","Very High",8517]
["5.10","High",8526]
["5.11","Low",8527]
["5.12","Medium",8528]
["5.13","High",8529]
["5.14","Very High",8530]
["5.15","Medium",8531]
["5.16","Very High",8532]
["5.17","Very High",8533]
["5.18","High",8534]
["5.19","Medium",8535]
["5.2","Very High",8518]
["5.20","Medium",8536]
["5.21","Medium",8537]
["5.22","High",8539]
["5.23","Very High",8540]
["5.24","Very High",8541]
["5.25","Medium",8542]
["5.26","Medium",8543]
["5.27","Medium",8544]
["5.28","Very High",8545]
["5.29","High",8546]
["5.3","Low",8519]
["5.30","High",8547]
["5.31","High",8548]
["5.32","High",8549]
["5.33","High",8550]
["5.34","Low",8551]
["5.35","Medium",8552]
["5.36","Low",8553]
["5.37","Low",8554]
["5.38","High",8555]
["5.39","Very High",8556]
["5.4","High",8520]
["5.40","Very High",8557]
["5.41","Very High",8558]
["5.42","Medium",8559]
["5.43","High",8560]
["5.44","High",8561]
["5.45","Medium",8564]
["5.46","Medium",8565]
["5.47","Medium",8566]
["5.48","Medium",8567]
["5.5","Low",8521]
["5.6","Low",8522]
["5.7","Medium",8523]
["5.8","Medium",8524]
["5.9","Very High",8525]
["5.99","High",8568]
["6.1","Medium",8348]
["6.10","Low",8357]
["6.11","High",8358]
["6.12","Medium",8359]
["6.13","Low",8360]
["6.14","High",8361]
["6.15","High",8362]
["6.16","Very High",8363]
["6.17","Very High",8364]
["6.18","Medium",8365]
["6.19","Low",8366]
["6.2","High",8349]
["6.20","Medium",8367]
["6.21","High",8368]
["6.22","Medium",8369]
["6.3","Low",8350]
["6.4","High",8351]
["6.5","Medium",8352]
["6.6","Medium",8353]
["6.7","High",8354]
["6.8","High",8355]
["6.9","Low",8356]
["6.99","High",8370]
["7.1","High",8371]
["7.10","High",8380]
["7.11","High",8381]
["7.12","High",8382]
["7.13","Medium",8383]
["7.14","Medium",8384]
["7.15","High",8385]
["7.16","High",8386]
["7.17","High",8387]
["7.2","High",8372]
["7.3","Low",8373]
["7.4","Low",8374]
["7.5","Low",8375]
["7.6","Medium",8376]
["7.7","Low",8377]
["7.8","High",8378]
["7.9","High",8379]
["7.99","High",8388]
["8.1","Very High",8569]
["8.10","Very High",8578]
["8.100","Low",11227]
["8.101","Medium",11228]
["8.102","Low",11229]
["8.103","Low",11230]
["8.104","Low",11231]
["8.105","Medium",11232]
["8.106","Medium",11233]
["8.107","Low",11234]
["8.108","High",11235]
["8.109","Very High",11236]
["8.11","Medium",8579]
["8.110","High",11237]
["8.111","Medium",11238]
["8.112","High",11239]
["8.113","Medium",11240]
["8.114","Low",11241]
["8.115","High",11242]
["8.116","Medium",11243]
["8.117","Medium",11244]
["8.118","Medium",11245]
["8.119","High",11246]
["8.12","Medium",8580]
["8.120","High",11247]
["8.121","Medium",11248]
["8.122","High",11249]
["8.123","High",11250]
["8.124","Low",11251]
["8.125","High",11252]
["8.126","Medium",11253]
["8.127","Medium",11254]
["8.13","Medium",8581]
["8.14","Very High",8582]
["8.15","High",8583]
["8.16","Very High",8584]
["8.17","Low",8585]
["8.18","High",8586]
["8.19","High",8587]
["8.199","High",11255]
["8.2","Medium",8570]
["8.20","Medium",8588]
["8.21","High",8589]
["8.22","Very High",8590]
["8.23","Medium",8591]
["8.24","Medium",8592]
["8.25","Very High",8593]
["8.26","High",8594]
["8.27","Medium",8595]
["8.28","Medium",8596]
["8.29","High",8598]
["8.3","Very High",8571]
["8.30","High",8599]
["8.31","High",8600]
["8.32","Low",8601]
["8.33","Medium",8602]
["8.34","High",8603]
["8.35","Medium",8604]
["8.36","Medium",8605]
["8.37","High",8607]
["8.38","Medium",8608]
["8.39","Medium",8609]
["8.4","Medium",8572]
["8.40","High",8610]
["8.41","Medium",8611]
["8.42","Medium",8612]
["8.43","Very High",8613]
["8.44","High",8615]
["8.45","High",8616]
["8.46","Very High",8617]
["8.47","Very High",8618]
["8.48","Medium",8619]
["8.49","High",8620]
["8.5","Very High",8573]
["8.50","Medium",8621]
["8.51","Low",8622]
["8.52","Low",8623]
["8.53","Low",8624]
["8.54","High",8625]
["8.55","Low",11182]
["8.56","Medium",11183]
["8.57","Medium",11184]
["8.58","High",11185]
["8.59","High",11186]
["8.6","Medium",8574]
["8.60","High",11187]
["8.61","Medium",11188]
["8.62","Very High",11189]
["8.63","High",11190]
["8.64","Medium",11191]
["8.65","Low",11192]
["8.66","High",11193]
["8.67","High",11194]
["8.68","High",11195]
["8.69","Medium",11196]
["8.7","High",8575]
["8.70","Medium",11197]
["8.71","Very High",11198]
["8.72","Medium",11199]
["8.73","Medium",11200]
["8.74","High",11201]
["8.75","Medium",11202]
["8.76","Medium",11203]
["8.77","Medium",11204]
["8.78","Medium",11205]
["8.79","Medium",11206]
["8.8","Medium",8576]
["8.80","Medium",11207]
["8.81","Low",11208]
["8.82","Medium",11209]
["8.83","Low",11210]
["8.84","Low",11211]
["8.85","Medium",11212]
["8.86","Medium",11213]
["8.87","Medium",11214]
["8.88","Low",11215]
["8.89","High",11216]
["8.9","High",8577]
["8.90","High",11217]
["8.91","High",11218]
["8.92","Medium",11219]
["8.93","Low",11220]
["8.94","Low",11221]
["8.95","Medium",11222]
["8.96","Medium",11223]
["8.97","Low",11224]
["8.98","High",11225]
["8.99","Medium",11226]
["9.1","Low",8390]
["9.10","Medium",8399]
["9.11","Medium",8400]
["9.12","Medium",8401]
["9.13","Low",8402]
["9.14","Medium",8403]
["9.15","Medium",8404]
["9.16","High",8405]
["9.17","High",8406]
["9.18","Low",8407]
["9.19","Low",8408]
["9.2","Very High",8391]
["9.20","Medium",8409]
["9.21","Medium",8410]
["9.22","Low",8411]
["9.23","Low",8412]
["9.24","Medium",8413]
["9.25","Low",8414]
["9.26","Low",8415]
["9.27","Low",8416]
["9.28","Medium",8417]
["9.29","Low",8418]
["9.3","Very High",8392]
["9.4","High",8393]
["9.5","High",8394]
["9.6","Low",8395]
["9.7","Medium",8396]
["9.8","Medium",8397]
["9.9","Medium",8398]
["9.99","High",8419]

{"sheet":"Equipment_list","index":7,"n_rows":28,"n_cols":3,"rows_kept":28,"cut":false,"hidden":true,"merged":[]}
["TITLE","Equipment_list_description","ID"]
["Accommodation",null,12]
["Cargo Mach.",null,13]
["Critical Equip.",null,16]
["Deck - Machinery",null,18]
["Deck - Mooring Machinery",null,15]
["Deck - Pipe / Fittings",null,20]
["Documentation",null,21]
["E/R - Air Comp.",null,8]
["E/R - Aux. Engine",null,4]
["E/R - Aux. Mach.",null,7]
["E/R - Boiler",null,5]
["E/R - Main Engine",null,3]
["E/R - Pipes/ valves & fittings",null,9]
["E/R - Pumps",null,32]
["E/R - Purifier",null,6]
["Elect. Mach. & Equip.",null,10]
["Hull & Tanks",null,19]
["Inert Gas",null,14]
["LSA / FFA",null,17]
["Miscellaneous",null,22]
["Navigation - DGPS / EPFS / AIS",null,28]
["Navigation - ECDIS",null,25]
["Navigation - Echo Sounder / Speed Log",null,26]
["Navigation - GMDSS & Communication",null,23]
["Navigation - Others",null,11]
["Navigation - RADAR",null,24]
["Navigation - VDR / BNWAS",null,30]

{"sheet":"PSC_MOU","index":8,"n_rows":11,"n_cols":3,"rows_kept":11,"cut":false,"hidden":true,"merged":[]}
["TITLE","PSC_MOU_description","ID"]
["Asia and the Pacific",null,2]
["Caribbean",null,4]
["Europe and the North Atlantic",null,1]
["Latin America",null,3]
["The Black Sea region",null,6]
["The Indian Ocean",null,8]
["The Mediterranean",null,7]
["The Riyadh MoU",null,9]
["USCG",null,10]
["West and Central Africa",null,5]

{"sheet":"Inspection_type","index":9,"n_rows":14,"n_cols":2,"rows_kept":14,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Bunkering Audit",14]
["Cargo Audit",17]
["Engineering Audit",16]
["ISM Audit",2]
["ISPS Audit",3]
["IT Audit",10]
["MLC Audit",1]
["Mooring Audit",9]
["Nav Audit / Verification",8]
["Onboard Training",18]
["PSC Inspection",4]
["Ship Staff Insp.",15]
["Suptd. Insp.",13]

{"sheet":"Deficiency_Cause","index":10,"n_rows":8,"n_cols":3,"rows_kept":8,"cut":false,"hidden":true,"merged":[]}
["TITLE","Deficiency_Cause_description","ID"]
["Behaviour Based",null,1]
["Equipment Related",null,4]
["External Factors",null,5]
["Human Error",null,7]
["Inappropriate Procedure",null,8]
["Industry Issue",null,6]
["Knowledge Based",null,3]

{"sheet":"Observer_code","index":11,"n_rows":3,"n_cols":3,"rows_kept":3,"cut":false,"hidden":true,"merged":[]}
["TITLE","Observer_code_description","ID"]
["Owner / Marine / Tech. Suptd.",null,3]
["Ship Staff",null,2]

{"sheet":"Status_code","index":12,"n_rows":6,"n_cols":3,"rows_kept":6,"cut":false,"hidden":true,"merged":[]}
["TITLE","Status_code_description","ID"]
["Completed",null,6]
["Deferred to D D",null,5]
["In progress",null,3]
["Not Started",null,2]
["Waiting spare",null,4]

{"sheet":"PSC_ref_no","index":13,"n_rows":19,"n_cols":2,"rows_kept":19,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Alarms",9]
["Cargo operations including equipment",7]
["Certificates & Documentation",2]
["Dangerous Goods",13]
["Emergency Systems",5]
["Fire safety",8]
["ISM",16]
["ISPS",17]
["Life saving appliances",12]
["MLC, 2006",18]
["Other",19]
["Pollution Prevention",15]
["Propulsion and auxiliary machinery",14]
["Radio communication",6]
["Safety of Navigation",11]
["Structural condition",3]
["Water/Weathertight condition",4]
["Working and Living Conditions",10]

{"sheet":"Risk_value_of_obs","index":14,"n_rows":1,"n_cols":2,"rows_kept":1,"cut":false,"hidden":true,"merged":[]}
["Risk Value of observation","ID"]

{"sheet":"Year","index":15,"n_rows":18,"n_cols":1,"rows_kept":18,"cut":false,"hidden":true,"merged":[]}
["Year"]
[2014]
[2015]
[2016]
[2017]
[2018]
[2019]
[2020]
[2021]
[2022]
[2023]
[2024]
[2025]
[2026]
[2027]
[2028]
[2029]
[2030]

{"sheet":"Month","index":16,"n_rows":13,"n_cols":1,"rows_kept":13,"cut":false,"hidden":true,"merged":[]}
["Month"]
["Jan"]
["Feb"]
["Mar"]
["Apr"]
["May"]
["Jun"]
["Jul"]
["Aug"]
["Sep"]
["Oct"]
["Nov"]
["Dec"]

{"sheet":"Date_","index":17,"n_rows":32,"n_cols":1,"rows_kept":32,"cut":false,"hidden":true,"merged":[]}
["Date"]
["01"]
["02"]
["03"]
["04"]
["05"]
["06"]
["07"]
["08"]
["09"]
[10]
[11]
[12]
[13]
[14]
[15]
[16]
[17]
[18]
[19]
[20]
[21]
[22]
[23]
[24]
[25]
[26]
[27]
[28]
[29]
[30]
[31]

{"sheet":"Sheet1","index":18,"n_rows":24,"n_cols":6,"rows_kept":24,"cut":false,"hidden":true,"merged":[]}
[]
[null,"ID","E",null,"Date Recorded",1]
[null,"UNIQUE ID","F",null,"Type of Deficiency",2]
[1,"Date Recorded","G",null,"Observer code",3]
["ignore","Vessel Type","H",null,"Type of Inspection",4]
[null,"Internal / External","I",null,"Description of Deficiency",5]
[null,"Drydock","J",null,"Equipment Categories",6]
[null,"Information Sharing","K",null,"Area of Observation",7]
[null,"Critical_item","L",null,"Deficiency Cause",8]
[null,"Deficiency Type","M",null,"VIQ Ref Number",9]
[null,"Deficiency Cause","N",null,"Risk Value of Obs",10]
[null,"Inspection Type","O",null,"PSC Ref Number",11]
[null,"Equipments","P",null,"PSC MOU ID",12]
[null,"VIQ Reference Number","Q",null,"Action Taken or Required",13]
[null,"Risk Value of the observation","R",null,"Target Date",14]
[null,"PSC Reference Number","S",null,"PO Ref No.",15]
[null,"PSC MOU","T",null,"Status Code",16]
[null,"Observer Code","U",null,"Date Completed",17]
[null,"Target Date","V",null,"Drydock",18]
[null,"Status Code","W",null,"Info Sharing",19]
[null,"Description of Deficiency","X",null,"Critical Item Flag",20]
[null,"Action taken / required","Y",null,"Audit Type",21]
[null,"PO ref no","Z"]
[null,"Date completed","AA"]

{"sheet":"Ship_information","index":19,"n_rows":2,"n_cols":4,"rows_kept":2,"cut":false,"hidden":true,"merged":[]}
["Ship_ID","Ship_Name","FILE_NAME","Export_Date"]
["30","DHT JAGUAR (03-05-2025)","30_1746269948786.xlsm","2025-07-01 09:07:71"]

{"sheet":"External_Deficiency_type","index":20,"n_rows":5,"n_cols":3,"rows_kept":5,"cut":false,"hidden":true,"merged":[]}
["TITLE","Type of deficiency_description","ID"]
["Condn of Class / Memo",null,5]
["Defect",null,1]
["Non Conformity",null,2]
["Observation",null,3]

{"sheet":"External_Inspection_type","index":21,"n_rows":11,"n_cols":2,"rows_kept":11,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Cargo Audit",17]
["Flag State Insp.",5]
["ISM Audit",2]
["ISPS Audit",3]
["MLC Audit",1]
["Nav Audit / Verification",8]
["OM Insp. (Eg. SIRE / CDI etc.)",6]
["Others (Eg. Insurance etc.)",12]
["PSC Inspection",4]
["Terminal Insp.",11]

{"sheet":"External_Observer_code","index":22,"n_rows":7,"n_cols":3,"rows_kept":7,"cut":false,"hidden":true,"merged":[]}
["TITLE","Observer_code_description","ID"]
["Class Surveyor",null,4]
["FSC Inspector",null,5]
["Others (Eg. Insurance etc.)",null,9]
["PSC Insp.",null,6]
["SIRE / CDI Insp.",null,8]
["Terminal Insp.",null,7]

{"sheet":"Sheet Version","index":23,"n_rows":2,"n_cols":2,"rows_kept":2,"cut":false,"hidden":true,"merged":[]}
["Version","Title"]
["2.0","Version 2.0"]