{"text_format":"1","workbook":"xlsx","n_sheets":24,"sheets":["Mainsheet","Completed","Calc","Areaofobs","Vessel_type","Deficiency_type","VIQrefno","Equipment_list","PSC_MOU","Inspection_type","Deficiency_Cause","Observer_code","Status_code","PSC_ref_no","Risk_value_of_obs","Year","Month","Date_","Sheet1","Ship_information","External_Deficiency_type","External_Inspection_type","External_Observer_code","Sheet Version"],"not_rendered":{"charts":0,"images":1,"macros":1,"external_links":0,"defined_names":12,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Mainsheet","index":0,"n_rows":44,"n_cols":28,"rows_kept":44,"cut":false,"hidden":false,"merged":[[10,8,10,9],[10,12,10,13],[12,6,12,27],[8,6,8,27]]}
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,"Defect - Damage Monitoring Sheet"]
[]
[null,null,null,null,null,null,null,"Date of Report","28-Aug-2025",null,null,"Ship Name","DHT SUNDARBANS (16-04-2025)"]
[]
[null,null,null,null,null,null,"VERSION : 2.0"]
[]
[]
[]
[null,null,null,"ID","SHIPSIDE UNIQUEID","UNIQUE ID","Date Recorded","Type of Deficiency","Observer code","Type of Inspection","Description of Deficiency","Equipment Categories","Area of Observation","Deficiency Cause","VIQ Ref Number","Risk Value of Obs","PSC Ref Number","PSC MOU ID","Action Taken or Required","Target Date","PO Ref No.","Status Code","Date Completed","Drydock","Info Sharing","Critical Item","Audit Type","Superintendent Remarks"]
[null,null,null,null,67996,"55_Wed Jan 15 2025 23:52:56 GMT+0800","2025-07-20T08:00:00","Defect","Ship Staff","Ship Staff Insp.","VRCS PRESSURE SWITCH FOR LP PUMP START & HP PUMP TRIP IS MALFUNCTIONING.","Cargo Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","RO SSUN250039 RAISED FOR VRCS PRESSURE SWITCH FOR LP PUMP START & HP PUMP TRIP","2025-10-20T08:00:00","SSUN250039","Waiting spare",null,"No","No","No","Internal","RO is approved. Same will be connected in next suitable port."]
[null,null,null,null,75569,"55_Mon Feb 10 2025 10:11:56 GMT+0800","2025-07-23T08:00:00","Defect","Ship Staff","Ship Staff Insp.","T/G condenser CSW pump discharge valve found not holding","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","The Discharge valve inspected and condition of the valve found poor. The valve needs to be renewed. requisition no.SSUN25011 , We have received the valve and waiting for opportunity.","2025-10-23T08:00:00","Requisition no. SSUN25011","In progress",null,"No","No","No","Internal","Pls create RO for new valve."]
[null,null,null,null,19822,"55_Sun Feb 09 2025 11:37:26 GMT+0800","2025-07-25T08:00:00","Defect","Ship Staff","Ship Staff Insp.","BWTS FLOW LEVEL SWITCH LS 1111 FOR ELECTROLIERS FOUND MALFUNCTIONING","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","BWTS FLOW LEVEL SWITCH LS 1111 FOR ELECTROLISERS AND RECTIFIER SAFETY NOT GIVING SIGNAL UPON CHECKS FOUND THAT SWITCH CONNECTION TERMINAL FULL OF WATER AND ALL CONNECTIONS IS BURNET AT PRESENT NO SPARES ON BORD FOR BWTS OPERATIONAL PURPOSE BYPASS THE FLOW SWITCH LS 1111 AND TESTED BWTS BALLAST OPERATIONS WORKING. SATISFACTORY.  RO - SSUN250071 RAISED","2025-10-25T08:00:00","SSUN250071","Waiting spare",null,"No","No","No","Internal","PO is approved. Same will be connected in next suitable port."]
[null,null,null,null,85662,"55_Sun Feb 16 2025 16:42:15 GMT+0800","2025-07-27T08:00:00","Defect","Ship Staff","Ship Staff Insp.","# 1 A/C compressor ACS - 2 HD controller is malfunctioning( working in only 1st stage, not cutting in to 2nd stage).","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","SSUN250063 raised & awaiting supply","2025-10-27T08:00:00","SSUN250063","Waiting spare",null,"No","No","No","Internal","PO is approved. Same will be connected in next port."]
[null,null,null,39978,null,"55_Fri Mar 21 2025 02:16:43 GMT+0000","2025-07-29T08:00:00","Observation","Ship Staff","Ship Staff Insp.","EGCS sea water pumps common outlet manifold is in poor state and double plate has been welded at some section to repair leak, The manifold is in difficult place to remove and shore workshop assistance is needed for completion of the job in short duration, Suggest workshop assistance during bunkering at Singapore around second week of November 2024.  2) EGCS Jet and Absorber unit sea water inlet pipes (distance pieces)  before casing and after valves need replacement. 3) EGCS absorber unit base plate welding seam is slightly leaking from one place and need repairs.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","EGCS sea water pumps common outlet manifold is in poor state and double plate has been welded at some section to repair leak, The manifold is in difficult place to remove and shore workshop assistance is needed for completion of the job in short duration, Suggest workshop assistance during bunkering at Singapore around second week of November 2024.  2) EGCS Jet and Absorber unit sea water inlet pipes (distance pieces)  before casing and after valves need replacement. 3) EGCS absorber unit base plate welding seam is slightly leaking from one place and need repairs.","2025-10-29T08:00:00","","Not Started",null,"No","No","No","Internal","Noted. Will plan during next singapore call."]
[null,null,null,null,94935,"55_Thu Mar 20 2025 14:33:39 GMT+0800","2025-03-11T08:00:00","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","M/E Viscosity controller is not operational.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","Office PO, awaiting for spare","2025-06-11T08:00:00","","Waiting spare",null,"No","No","No","Internal","Please create RO. This no RO available."]
[null,null,null,null,44757,"0_Wed Mar 26 2025 06:50:53 GMT+0800","2025-03-20T08:00:00","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Remote gauging readout for Forepeak \nis erratic. To rectify fault","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","Troubleshooting in progress. Requisition SSUN250127 raised for the same. ","2025-06-20T08:00:00","SSUN250127","Waiting spare",null,"No","No","No","Internal","Carry out troubleshooting and order for required pares. Pls liaise with autoelec dept, if required."]
[null,null,null,null,44885,"55_Wed Mar 26 2025 06:49:43 GMT+0800","2025-03-20T08:00:00","Non Conformity","Owner / Marine / Tech. Suptd.","Suptd. Insp.","PV valves vacuum side noted have teflon ring inserts to\nprevent leakage. Same to be removed and PV valves\nrestored to design","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","PV valves vacuum side to be overhauled and  PV valves\nto be restored to design.","2025-06-20T08:00:00","","Not Started",null,"No","No","No","Internal","Carry out troubleshooting as required and revert."]
[null,null,null,null,60439,"0_Wed Mar 26 2025 07:04:59 GMT+0800","2025-03-20T08:00:00","Observation","Owner / Marine / Tech. Suptd.","Cargo Audit","Port side aft 10t provision crane has hydraulic leak from\nram. To rectify","Deck - Machinery","Cargo / Ballast Systems","Equipment Related","","","","","Spares received against PO SSUN250069 , AWAITING OPPORTUNITY.","2025-06-20T08:00:00","SSUN250069","In progress",null,"No","No","No","Internal","PO is approved. Same will be connected at next suitable port."]
[null,null,null,null,36552,"0_Wed Mar 26 2025 07:03:33 GMT+0800","2025-03-20T08:00:00","Observation","Owner / Marine / Tech. Suptd.","Cargo Audit","Both 20t HHC observed hook hoisting speed is slower than\ndesign. To verify and re-set.","Deck - Machinery","Cargo / Ballast Systems","Equipment Related","","","","","Requires health check and speed adjustment of HHC.","2025-06-20T08:00:00","","Not Started",null,"No","No","No","Internal","Pls verify and revert."]
[null,null,null,null,54078,"55_Sat Apr 12 2025 02:36:06 GMT+0800","2025-08-02T08:00:00","Defect","Ship Staff","Ship Staff Insp.","A crack exists in shell plating of WHRU(Economizer) casing where HP and LP section meet. Due to this crack exhaust gas leaks off in ER casing during WHRS operation.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","Shell lagging to remove and economizer shell plating to check for extension and extend of crack, A plate to be welded on casing plate to stop exhaust gas leak, Prior work all lagging material to be removed and area to be clean. Again workshop assistance is require to carry out said job.","2025-11-02T08:00:00","","In progress",null,"No","No","No","Internal","Noted,  plan the Job during Singapore call. \nPrepare a job plan with staging required if any and order for the materials required for repair."]
[null,null,null,null,58053,"55_Sat Apr 12 2025 02:40:46 GMT+0800","2025-08-02T08:00:00","Defect","Ship Staff","Ship Staff Insp.","BWTS- BT 2213 Filter Bypass valve cannot operate remotely from CCR","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","","","","","Valve is not opening from CCR but can open locally from Pumproom in local mode. (if need to open from pumproom we have to use manual hydraulic pump","2025-11-02T08:00:00","","In progress",null,"No","No","No","Internal"]
[null,null,null,null,71680,"55_Sat Apr 12 2025 02:43:13 GMT+0800","2025-08-02T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Mid ship draft gauge valve need to be renewed, actuator in 3P WBT is not operational. New Gate valve with Actuator received in Jan 2024 with different design of actuator hence we have to change the full valve only.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","","","","","For changing the full valve we required diver to put plug or can be done in drydock. But CCR Readout is working satisfactory & showing midship draft.","2025-11-02T08:00:00","SSUN235066","Not Started",null,"No","No","No","Internal"]
[null,null,null,null,75155,"0_Sat Apr 12 2025 02:54:02 GMT+0800","2025-08-05T08:00:00","Defect","Ship Staff","Ship Staff Insp.","EGCS absorber level control valve 2280A kept open in manual, upon inspection found the SW leakage from the valve spindle to the actuator side making it inoperable. The POSITIONER SIPART PS 2 found to be working satisfactory.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","The Actuator inspected and the condition of the actuator found in poor condition and needs to be renewed. Requisition 250165 has been raised for new actuator.","2025-11-05T08:00:00","SSUN240232","In progress",null,"No","No","No","Internal"]
[null,null,null,null,13299,"55_Sat Apr 12 2025 02:51:47 GMT+0800","2025-08-05T08:00:00","Defect","Ship Staff","Ship Staff Insp.","BWTS- BT 2212 Filter Outlet valve cannot operate remotely from CCR","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","6.21","High","","","Valve is now opening from CCR but cannot open locally from Pumproom in local mode. (if need to open from pumproom we have to use manual hydraulic pump, Display for the valve in pumproom still not working) . ","2025-11-05T08:00:00","","In progress",null,"No","No","No","Internal"]
[null,null,null,null,97935,"0_Sat Apr 12 2025 02:58:12 GMT+0800","2025-08-07T08:00:00","Defect","Ship Staff","Ship Staff Insp.","WHRS exhaust gas temperature sensor #12 for HP and LP, and sensor #22 is faulty.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","RO - SSUN250111 raised, awaiting for supply.","2025-11-07T08:00:00","Requisition SSUN250111 raised for the same, ","Waiting spare",null,"No","No","No","Internal"]
[null,null,null,null,98130,"0_Sat Apr 12 2025 03:04:20 GMT+0800","2025-08-10T08:00:00","Defect","Ship Staff","Ship Staff Insp.","ME rail unit supports welding crack observed & rail securing u clamps found broken.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","U clamps fabricated & fitted. Welding cracks to be repaired at the earliest opportunity.","2025-11-10T08:00:00","","Not Started",null,"No","No","No","Internal"]
[null,null,null,null,45085,"0_Sat Apr 12 2025 03:05:42 GMT+0800","2025-08-10T08:00:00","Defect","Ship Staff","Ship Staff Insp.","ME # 2 scavenge air inlet casing has developed hair line crack in the welding seam","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","The leakage is arrested by lagging material at present, same will be renewed once the ME is stopped.","2025-11-10T08:00:00","","In progress",null,"No","No","No","Internal"]
[null,null,null,null,17395,"0_Sat Apr 12 2025 03:07:38 GMT+0800","2025-08-13T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Exhaust gas leaking from WHRS casing, lagging damage observed at several places.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","Need to identify the location of the leak.","2025-11-13T08:00:00","","In progress",null,"No","No","No","Internal"]
[null,null,null,null,50784,"0_Sat Apr 12 2025 03:14:01 GMT+0800","2025-08-13T08:00:00","Defect","Ship Staff","Ship Staff Insp.","STBD Windlass gear engaging/Clutching lever Hydraulic cylinder not working","Deck - Mooring Machinery","Mooring","Equipment Related","9.20","Medium","","","RO SSUN250193 raised for the same.","2025-11-13T08:00:00","SSUN250193","Waiting spare",null,"No","No","No","Internal"]
[null,null,null,null,31482,"0_Sun Jun 15 2025 15:48:30 GMT+0800","2025-05-29T08:00:00","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","All winches oil sight glass to be cleaned.","Deck - Machinery","Mooring","Equipment Related","","","","","All sight glass cleaned but few of them seems opaque. PO: SSUN250117 waiting for spare.","2025-08-29T08:00:00","PO: SSUN250117","Waiting spare",null,"No","No","No","Internal"]
[null,null,null,null,29317,"55_Wed Aug 20 2025 15:59:27 GMT+0800","2025-08-16T08:00:00","Defect","Ship Staff","Ship Staff Insp.","The Rectifier no.3 is not starting while the BWTS is in operation. Manual and auto operation of the rectifier is not working.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","System tried out and is found working on other two rectifiers no.1 and no.2 , while awaiting further instructions for trouble shooting.","2025-11-16T08:00:00","","In progress",null,"No","No","No","Internal"]
[null,null,null,null,23825,"55_Wed Aug 20 2025 16:06:43 GMT+0800","2025-08-16T08:00:00","Defect","Ship Staff","Ship Staff Insp.","The Oil Content Monitor sensor for the Main Engine Jacket water defective. The sensor needs to be renewed.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Trouble shooting carried out and found that the sensor defective and needs to be renewed. Requisition SSUN250184 raised for new sensor.","2025-11-16T08:00:00","SSUN250184","Waiting spare",null,"No","No","No","Internal"]
[null,null,null,null,31534,"55_Wed Aug 20 2025 16:14:45 GMT+0800","2025-08-18T08:00:00","Defect","Ship Staff","Ship Staff Insp.","The Fixed Gas Detection system for the Water Ballast tank is found malfunctioning and internal leakage alarm getting activated after every 6 hours and needs to be reset.","Elect. Mach. & Equip.","Safety / LSA / FFA","Equipment Related","","","","","Trouble shooting carried out and as per the correspondence with the office,   RIOK 40 PCB and other PCBs’s for the SW2020 FGDS will be supplied during the next Singapore call.","2025-11-18T08:00:00","","Waiting spare",null,"No","No","No","Internal"]
[null,null,null,null,40748,"55_Wed Aug 20 2025 16:19:14 GMT+0800","2025-08-20T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Soot blower lance no.1 and no.3 of the LP section of the WHRS and no.5 of the HP section found wasted and needs to be renewed.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","Soot blower lance no.1 and no.3 of the LP section of the WHRS and no.5 of the HP section found wasted and needs to be renewed. Requisition SSUN250188 raised for the soot blower lance.","2025-11-20T08:00:00","SSUN250188","Waiting spare",null,"No","No","No","Internal"]
[null,null,null,null,85391,"55_Thu Aug 28 2025 18:29:22 GMT+0800","2025-08-04T08:00:00","Defect","Ship Staff","Ship Staff Insp.","BWTS AP tank filter bypass valve BT3213 PCB is faulty","Miscellaneous","Cargo / Ballast Systems","Equipment Related","6.21","High","","","Requisition SSUN250035 raised , awaiting for spare","2025-11-04T08:00:00","SSUN250035","Waiting spare",null,"No","No","No","Internal"]
[null,null,null,null,87057,"55_Thu Aug 28 2025 18:36:29 GMT+0800","2025-08-04T08:00:00","Defect","Ship Staff","Ship Staff Insp.","BWTS AP TANK TRO UNIT PANEL PCB IS FAULTY","Elect. Mach. & Equip.","Cargo / Ballast Systems","Equipment Related","6.12","Medium","","","REQUISITION SSUN250035 raised , awaiting for spare","2025-11-04T08:00:00","SSUN250035","Waiting spare",null,"No","No","No","Internal"]

{"sheet":"Completed","index":1,"n_rows":537,"n_cols":28,"rows_kept":537,"cut":false,"hidden":false,"merged":[[10,8,10,9],[10,12,10,13],[12,6,12,27],[8,6,8,27]]}
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,"Defect - Damage Monitoring Sheet"]
[]
[null,null,null,null,null,null,null,"Date of Report","28-Aug-2025",null,null,"Ship Name","DHT SUNDARBANS (16-04-2025)"]
[]
[null,null,null,null,null,null,"VERSION : 2.0"]
[]
[]
[]
[null,null,null,"ID","SHIPSIDE UNIQUEID","UNIQUE ID","Date Recorded","Type of Deficiency","Observer code","Type of Inspection","Description of Deficiency","Equipment Categories","Area of Observation","Deficiency Cause","VIQ Ref Number","Risk Value of Obs","PSC Ref Number","PSC MOU ID","Action Taken or Required","Target Date","PO Ref No.","Status Code","Date Completed","Drydock","Info Sharing","Critical Item","Audit Type","Superintendent Remarks"]
[null,null,null,24453,null,"55_20/3/2022 4:39:59 pm","2022-01-22T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","ME JCW Temperature Control Valve Position Sensor Fail\t\t\t\t","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.2","Low","","","We have replaced the valve positioner and alarm has cleared.","2022-05-17T23:59:09.999","SSUN220038","Completed","2022-05-22T23:59:09.999","No","No","No","Internal"]
[null,null,null,26352,50895,"55_Tue Jul 12 2022 02:02:45 GMT+0800","2022-02-02T23:59:09.999","Observation","Ship Staff","Ship Staff Insp.","VDR RCU UNIT PCB Eject button defective, New PCB received & replaced but due to Error in installation, Old one placed back in use again as per Instructions from office. New MCB on board. However New MCB onboard need to be configured for all channels inputs and that only service engineer can do. ","Navigation - Others","Navigation","Equipment Related","4.7","High","","","Awaiting service Engineer attendance. Office to be informed prior convenient port call for attendance of service Engineer.  So that new PCB onboard can be programmed for all input channels and can be fixed.\n06 Sep 2022 / Action Taken - New PCB installed. Remote troubleshooting and programming carried out by Service Engineer. Eject button & VDR working in good order . Job Completed.","2022-10-12T23:59:09.999","N/A - Office to be informed prior convenient port call for attendance of service Engineer. ","Completed","2022-08-20T23:59:09.999","No","No","No","Internal"]
[null,null,null,26354,34778,"55_Tue Jul 12 2022 02:16:00 GMT+0800","2022-02-02T23:59:09.999","Critical Equipment","Ship Staff","Ship Staff Insp.","ECDIS fitted onboard 2 x JRC 901-B AND USED AS PRIMARY MEANS OF Navigation SSD last replaced July 2022. \nNo spare Pre-Programmed SSD's onboard as required under critical spare part list of company.","Navigation - ECDIS","Navigation","Equipment Related","","","","","Spare pre programmed SSD's not required , since As per the all makers, if vessel is equipped with dual ECDIS, no additional spares to be maintained.","2022-10-12T23:59:09.999","","Completed","2022-09-20T23:59:09.999","No","No","No","Internal"]
[null,null,null,24351,null,"55_1/3/2022 4:26:07 am","2022-02-07T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","Engine room skylight mooring wire found to have broken strands.","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","Equipment Related","5.47","Medium","","","Wire replaced.","2022-04-18T23:59:09.999","","Completed","2022-03-03T23:59:09.999","No","No","No","Internal"]
[null,null,null,24352,null,"55_5/3/2022 9:43:01 pm","2022-02-07T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","Various tap fittings in accomodation found to be leaking as reported by crew in Safety meeting","Accommodation","MLC Related","Equipment Related","11.13","Low","","","Requistion received through SSUN220050 and leaking taps renewed.","2022-05-09T23:59:09.999","","Completed","2022-04-01T23:59:09.999","No","No","No","Internal"]
[null,null,null,24353,null,"55_6/3/2022 1:50:14 pm","2022-02-08T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","FCV 1211 is not operating by remotely. Drive motor for the same was burnt. Currently FCV 1211 is operated manually.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","6.21","High","","","Drive motor received, job completed. ","2022-11-30T23:59:09.999","SSUN220035","Completed","2022-09-22T23:59:09.999","No","No","No","Internal","Raise requisition for drive motor ASAP."]
[null,null,null,24354,null,"55_6/3/2022 2:31:27 pm","2022-02-08T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","Port and stbd accommodation ladder lashing guide are not in good condition (rubber guides on which wire lashing is resting).","Deck - Pipe / Fittings","General Appearance","Equipment Related","5.47","Medium","","","Lashing guide ordered and received on board.\nSame has been renewed. Job completed.\n","2022-05-08T23:59:09.999","","Completed","2022-04-21T23:59:09.999","No","No","No","Internal","Noted. Close defect after renewing same."]
[null,null,null,24350,null,"55_5/3/2022 10:03:02 pm","2022-02-09T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","Electrical insulation matt found to be missing at various panels in Engine room.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.24","Low","","","Electrical insulation matt at missing locations installed.","2022-03-11T23:59:09.999","","Completed","2022-02-27T23:59:09.999","No","No","No","Internal","Mat supplied at DD. Close defect after putting at missing area."]
[null,null,null,24355,null,"55_5/3/2022 9:33:12 pm","2022-02-09T23:59:09.999","Observation","Ship Staff","Ship Staff Insp.","Loose items in Engine room not secured.","Miscellaneous","Eng. / Strg. Comp.","External Factors","5.11","Low","","","All loose items have been be shifted to their respective stowage  proper location and secured.","2022-03-09T23:59:09.999","","Completed","2022-02-19T23:59:09.999","No","No","No","Internal","Noted."]
[null,null,null,24356,null,"55_5/3/2022 9:47:01 pm","2022-02-09T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","Various doors including accomodation and purifier room door the holding latches screw found to be missing.","Accommodation,E/R - Purifier","Safety / LSA / FFA","Equipment Related","5.35","Medium","","","Missing screw for latches installed and door closing function tested for proper closing.","2022-04-09T23:59:09.999","","Completed","2022-02-23T23:59:09.999","No","No","No","Internal","Noted."]
[null,null,null,24357,null,"55_5/3/2022 9:50:37 pm","2022-02-09T23:59:09.999","Critical Equipment,Observation","Ship Staff","Ship Staff Insp.","Critical spare parts found to be missing and also critical spare part inventory to be updated in PAL.","E/R - Main Engine,Elect. Mach. & Equip.","Emgcy. Systems","Equipment Related","10.13","Very High","","","Missing critical spare parts to be requested upon taking complete inventory of critical spare parts. Closing as all spares ordered from vessel as well approved by office","2022-05-11T23:59:09.999","SSUN220007,SSUN220015,SSUN220016,SSUN220017,SSUN220018,SSUN220019,SSUN220020,SSUN220021,SSUN220022,S","Completed","2022-03-31T23:59:09.999","No","No","No","Internal"]
[null,null,null,24358,null,"55_5/3/2022 9:55:52 pm","2022-02-09T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","Laundry drying room thermostat not cutting off.","Accommodation","MLC Related","Equipment Related","11.14","Medium","","","Thermostat received and installed. job completed.","2022-05-01T23:59:09.999","SSUN220034","Completed","2022-05-01T23:59:09.999","No","No","No","Internal","Raise requisition."]
[null,null,null,24359,null,"55_5/3/2022 9:59:53 pm","2022-02-09T23:59:09.999","Observation","Ship Staff","Ship Staff Insp.","EGCS side shell renewal and various stubb piece renewed in Engine room and same area needs to be derusted and painting including funnel top deck plate.","Hull & Tanks","Structural Condn. / WT integrity ","Equipment Related","10.31","Very High","","","Area needs to be derusted and painted.","2022-03-11T23:59:09.999","","Completed","2022-02-24T23:59:09.999","No","No","No","Internal","Noted."]
[null,null,null,24360,null,"55_5/3/2022 10:07:37 pm","2022-02-09T23:59:09.999","Other","Ship Staff","Ship Staff Insp.","ECA Book not available onboard.","Miscellaneous","MARPOL Related","Industry Issue","10.5","Low","","","ECA book received and updated","2022-04-11T23:59:09.999","","Completed","2022-03-27T23:59:09.999","No","No","No","Internal"]
[null,null,null,24361,null,"55_5/3/2022 10:25:49 pm","2022-02-09T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","WHRS cladding insulation material found to be missing and same needs to be installed.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.19","Very High","","","yard fabricated insulation cladding cover and given to ship, same installed in place.","2022-04-11T23:59:09.999","Waiting for the engine to be stopped for enabling installation.","Completed","2022-04-01T23:59:09.999","No","No","No","Internal"]
[null,null,null,24362,null,"55_5/3/2022 10:33:34 pm","2022-02-09T23:59:09.999","Observation","Ship Staff","Ship Staff Insp.","Scrubber room not fitted with engine room alarm extension.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.2","Low","","","Alarm signal light and cable procured in DD and same installed. Tested operation and found satisfactory.","2022-04-16T23:59:09.999","","Completed","2022-04-16T23:59:09.999","No","No","No","Internal","Noted."]
[null,null,null,24363,null,"55_5/3/2022 10:42:44 pm","2022-02-09T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","High pressure pipe connected upon completion of decarb not secured with antisplash tape.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.19","Very High","","","Potential areas of splash to be protected with anti splash tape same installed and completed.","2022-04-10T23:59:09.999","","Completed","2022-04-01T23:59:09.999","No","No","No","Internal"]
[null,null,null,24454,null,"55_20/3/2022 2:53:05 pm","2022-02-10T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","Reported Garbage Compactor not opertional","Deck - Machinery","General Appearance","Equipment Related","6.2","High","","","NEW GARBAGE COMPACTOR INSTALLED","2022-09-11T23:59:09.999","SSUN220040","Completed","2022-09-21T23:59:09.999","No","No","No","Internal"]
[null,null,null,24455,null,"55_20/3/2022 4:53:22 pm","2022-02-10T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","Fault alarm was received on ER OMD Panel for Boiler Area #2","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.35","Medium","","","Spares received and same replaced and job completed.","2022-05-13T23:59:09.999","SSUN220039","Completed","2022-05-22T23:59:09.999","No","No","No","Internal"]
[null,null,null,25518,16952,"55_Tue May 31 2022 08:20:33 GMT+0800","2022-02-10T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","AUX DG TC COMPRESSOR WHEEL FOUND CHIPPED , EFFICIENCY OF TC NOT RELIABLE","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","SPARE TC CARTRIDGE REQUESTED. SAME INSTALLED","2022-05-13T23:59:09.999","STAI150016/2","Completed","2022-05-02T23:59:09.999","No","No","No","Internal"]
[null,null,null,24457,null,"55_20/3/2022 3:10:00 pm","2022-02-11T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","Bosun store water mist system repeater panel on bridge showing no indication.\t","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.35","Medium","","","PCB received and renewed.","2022-06-15T23:59:09.999","SSUN220032","Completed","2022-05-22T23:59:09.999","No","No","No","Internal"]
[null,null,null,24456,null,"55_20/3/2022 4:17:31 pm","2022-02-14T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","Back-up UPS for S-Band RADAR and Fire Fighting CO2 system was operational\t\t\t","LSA / FFA,Navigation - RADAR","Navigation","Equipment Related","","","","","Both UPS was bypassed to make the system online, S band radar spares received and installed. Awaiting spare for Co2 ups.\nNEW UPS RECEIVED installed","2022-09-11T23:59:09.999","SSUN220036","Completed","2022-09-28T23:59:09.999","No","No","No","Internal"]
[null,null,null,24842,null,"55_31/3/2022 11:02:04 am","2022-02-27T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","Fault with fire detection system due to faulty short circuit isolator.","Critical Equip.,LSA / FFA","Eng. / Strg. Comp.","Equipment Related","5.39","Very High","","","Informed office and the electrical department provided short circuit isolator in singapore on 27/03/2022 same installed and found fault alarm is clear.","2022-04-23T23:59:09.999","","Completed","2022-03-10T23:59:09.999","No","No","No","Internal"]
[null,null,null,24839,null,"55_31/3/2022 12:56:19 pm","2022-03-06T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","Topping up generator monthly outines tried out, noticed sw valve not holding as well one of the flame sensor is faulty.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","8.25","Very High","","","SW valve renewed.","2022-07-08T23:59:09.999","","Completed","2022-03-29T23:59:09.999","No","No","No","Internal"]
[null,null,null,24840,null,"55_31/3/2022 11:11:35 am","2022-03-11T23:59:09.999","Critical Equipment,Defect","Ship Staff","Ship Staff Insp.","Navigational light control panel though all lights were of “ON” indication without alarms in the panel.but, actually in real scenario no navigational lights present in mast head in monkey island,fwd mast, side light and stern lights.","Navigation - Others","Navigation","Equipment Related","4.8","Medium","","","New panel received & Renewed - tested & working in good order. Job Completed","2022-09-11T23:59:09.999","New panel received & Renewed - tested & working in good order. Job Completed","Completed","2022-08-19T23:59:09.999","No","No","No","Internal"]
[null,null,null,24841,null,"55_31/3/2022 1:00:09 pm","2022-03-11T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","Port side provision controller display had no indications, though there is no display indications the functionality of the crane controller is in good order. ","Miscellaneous","Structural Condn. / WT integrity ","Equipment Related","8.5","Very High","","","Controller replaced and job completed.","2022-07-18T23:59:09.999","","Completed","2022-04-03T23:59:09.999","No","No","No","Internal"]
[null,null,null,25513,83707,"55_Tue May 03 2022 22:23:29 GMT+0800","2022-03-13T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","MAIN ENGINE FUEL OIL HEATER #2 FOUND LEAKING ","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.1","Medium","","","FUEL OIL HEATER STACK REMOVED AND GASKET CHANGED,","2022-04-16T23:59:09.999","","Completed","2022-04-13T23:59:09.999","No","No","No","Internal"]
[null,null,null,25512,62197,"55_Sun May 01 2022 14:10:21 GMT+0800","2022-03-27T23:59:09.999","Observation","Ship Staff","Ship Staff Insp.","No 1 ME Fuel pump high pressure pipe connection found to have minor leaks","E/R - Main Engine,E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","High pressure pipe disconnected and found one O-ring to be damaged.  Same replaced and assembled back observed to find leakage to be stopped.","2022-05-07T23:59:09.999","","Completed","2022-04-10T23:59:09.999","No","No","No","Internal"]
[null,null,null,25510,18580,"55_Sun May 01 2022 16:40:06 GMT+0800","2022-04-12T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","ME DGU CAN A FAILURE","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.1","Medium","","","Service engineer attended in San Diego.  All CAN A and CAN B connections were swapped in E25 box. DGU AL module was replaced. issue rectified.","2022-07-13T23:59:09.999","SSUN225090","Completed","2022-05-22T23:59:09.999","No","No","No","Internal"]
[null,null,null,25519,13882,"55_Tue May 31 2022 08:22:47 GMT+0800","2022-04-12T23:59:09.999","Critical Equipment","Ship Staff","Ship Staff Insp.","SCRUBBER ROOM FIRE DAMPER HARD TO OPERATE","LSA / FFA","Eng. / Strg. Comp.","Equipment Related","5.35","Medium","","","DAMPER TO OVERHAUL AND MAKE FREE TO OPERATE","2022-05-12T23:59:09.999","","Completed","2022-05-11T23:59:09.999","No","No","No","Internal"]
[null,null,null,25514,57835,"55_Thu May 26 2022 12:19:35 GMT+0800","2022-04-13T23:59:09.999","Observation","Ship Staff","Ship Staff Insp.","Doppler log repeater display on Bridge front not clearly readable / visible  in the day-light with maximum brilliance. ","Navigation - Echo Sounder / Speed Log","Navigation","Equipment Related","4.7","High","","","New display ordered and replaced.","2022-05-01T23:59:09.999","SSUN225078","Completed","2022-04-29T23:59:09.999","No","No","No","Internal"]
[null,null,null,25515,51330,"55_Thu May 26 2022 12:29:39 GMT+0800","2022-04-13T23:59:09.999","Observation","Ship Staff","Ship Staff Insp.","MF/ HF Ariel securing clamp was observed missing during monthly test/checks of the equipment as per PMS schedule.","Navigation - GMDSS & Communication","Navigation","Equipment Related","4.7","High","","","MF/ HF Ariel securing clamp renewed.","2022-04-16T23:59:09.999","","Completed","2022-04-14T23:59:09.999","No","No","No","Internal"]
[null,null,null,26353,38287,"55_Tue Jul 12 2022 02:08:58 GMT+0800","2022-04-16T23:59:09.999","Observation","Ship Staff","Ship Staff Insp.","AIS is Unable to switch to LOW TX power (As Required by ISGOTT & Local port requirements)","Navigation - DGPS / EPFS / AIS","Navigation","Equipment Related","4.7","High","","","AIS software updated by shore on team viewer and AIS can be switched to LOW power .","2022-10-12T23:59:09.999","N/A","Completed","2022-07-17T23:59:09.999","No","No","No","Internal"]
[null,null,null,25517,66428,"55_Fri May 27 2022 03:16:27 GMT+0800","2022-04-21T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","4C COT overfill alarm not operational.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.14","Very High","","","Requisition made for Magnet in float assembly.\nReceived magnet and same has been renewed.\nOverfill alarm operational, job completed.\n","2022-05-02T23:59:09.999","SSUN220051","Completed","2022-04-30T23:59:09.999","No","No","No","Internal"]
[null,null,null,25516,71133,"55_Fri May 27 2022 02:52:35 GMT+0800","2022-04-26T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","Analyze pump internal leakage alarm on Pump room fixed gas detection system.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.46","Very High","","","Analyze Pump overhauled and renewed flow switch. Job completed. \nNo alarm on Pump room fixed gas detection system \n","2022-04-30T23:59:09.999","","Completed","2022-04-29T23:59:09.999","No","No","No","Internal"]
[null,null,null,25511,61845,"55_Tue May 31 2022 08:24:42 GMT+0800","2022-05-04T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","#1 FWG EJECTOR NOZZLE WORN, SHELL TEMP HIGH DUE TO LESS VACUUM","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","ejector renewed.\nvacuum is good now with fwg production 25mt","2022-09-12T23:59:09.999","SSUN220096","Completed","2022-09-18T23:59:09.999","No","No","No","Internal"]
[null,null,null,25509,70470,"55_Tue May 31 2022 08:26:30 GMT+0800","2022-05-05T23:59:09.999","Defect,Observation","Ship Staff","Ship Staff Insp.","WHRS MANHOLE GASKETS HAVE LEAK. THREADS FOR SECURING STUDA DAMGED","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Manhole gaskets renewed on WHRS for 6 no doors.","2022-08-05T23:59:09.999","","Completed","2022-05-26T23:59:09.999","No","No","No","Internal"]
[null,null,null,25633,61687,"55_Wed Jun 15 2022 02:20:34 GMT+0800","2022-05-14T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","M/E Tachometer no 1 and no 2 showing eratic reading when engine stopped.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","TACHOMETER CONNECTIONS RE CHECKED AND MADE CORRECT SAME WORKING.","2022-09-12T23:59:09.999","SSUN220058","Completed","2022-09-25T23:59:09.999","No","No","No","Internal"]
[null,null,null,25634,89448,"0_Wed Jun 15 2022 02:26:06 GMT+0800","2022-05-14T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","Common rail box tested for cracks and found few cracks and action needs to be taken.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Crack end punched in order to arrest the cracks.","2022-08-14T23:59:09.999","","Completed","2022-06-02T23:59:09.999","No","No","No","Internal"]
[null,null,null,25846,28192,"55_Mon Jun 20 2022 21:19:50 GMT+0800","2022-05-18T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","During the pressure testing it was observed that the Cargo Line No. 3 to IG Connection T-Piece was leaking. Same was fully tightened up and the leak was stopped.\nHowever suspect the Cargo Line No. 3 Valve to IG Line (OD-339) is suspected to be leaking. The line was re-pressurized to 11.0 bars and confirmed no leaks were observed during the time of inspection.\n","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.11","Medium","","","Renewed seat ring of valve OD-339, job completed.","2022-06-11T23:59:09.999","","Completed","2022-06-02T23:59:09.999","No","No","No","Internal"]
[null,null,null,25635,92117,"55_Wed Jun 15 2022 02:29:09 GMT+0800","2022-05-22T23:59:09.999","Observation","Ship Staff","Ship Staff Insp.","WIO sensor installed along with BWMS is decommissioned. Need to install new type WIO sensor.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Office to follow up to supply new type Water in oil sensor. once received same to be installed and an mimic in aconis to be created with aconis engineer.","2022-09-21T23:59:09.999","","Completed","2022-09-17T23:59:09.999","No","No","No","Internal"]
[null,null,null,25636,73085,"0_Wed Jun 15 2022 02:30:41 GMT+0800","2022-05-22T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","M/E top brazing no 4 is leaking.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","M/E top brazing no 4 needs to be overhauled. Spares are already onboard.","2022-08-22T23:59:09.999","","Completed","2022-07-09T23:59:09.999","No","No","No","Internal"]
[null,null,null,25637,81536,"55_Wed Jun 15 2022 02:33:24 GMT+0800","2022-05-22T23:59:09.999","Observation","Ship Staff","Ship Staff Insp.","M/E ICO lube 440 volt low insulation alarm comes when started.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Isolation transformer has been supplied to vessel and pending installation, same needs to be installed to clear alarm// ","2022-08-22T23:59:09.999","","Completed","2022-06-01T23:59:09.999","No","No","No","Internal"]
[null,null,null,25639,47889,"0_Wed Jun 15 2022 02:40:16 GMT+0800","2022-05-22T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","EGCS gas analyzer has chopper motor failure alarms","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Communication with maker spare parts ordered.. Gas analyser and service attendance arranged through SSUN225094","2022-09-21T23:59:09.999","SSUN225094","Completed","2022-09-15T23:59:09.999","No","No","No","Internal"]
[null,null,null,25641,49623,"0_Wed Jun 15 2022 02:53:28 GMT+0800","2022-05-22T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","We have noticed quantity discrepancy with Bilge guard flowmeter.\nTotal quantity discharged overboard recorded in Bilge guard is less than the actual quantity pumped overboard. We are recording actual quantity in ORB with reference to our manual sounding.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","QUANTITIES ARE CHECKED DURING LAST OPERATIONS AND FOUND NOT MUCH DIFFERENCE, UNDER MONITORING.","2023-06-19T23:59:09.999","SSUN230037","Completed","2023-06-11T23:59:09.999","No","No","No","Internal"]
[null,null,null,25642,72855,"55_Wed Jun 15 2022 05:05:16 GMT+0800","2022-05-22T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","One of the cargo pressure transmitter local display not visible.\n\n","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.41","Medium","","","Pressure transmitter for cargo manifold ordered through SSUN220071 SAME REPLACED AND SYSTEM BACK TO NORMAL","2022-09-18T23:59:09.999","SSUN220071","Completed","2022-09-26T23:59:09.999","No","No","No","Internal"]
[null,null,null,25643,11488,"55_Wed Jun 15 2022 05:11:11 GMT+0800","2022-05-22T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","Rosemount WSU one of the CPU has failed same ordered and awaiting spare SSUN225084. Communication with maker in progress backup file sent to maker as per request","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.70","Medium","","","Troubleshooting steps taken as per  service technician , Both WSU of Rosemount working satisfactorily","2022-08-22T23:59:09.999","","Completed","2022-08-07T23:59:09.999","No","No","No","Internal"]
[null,null,null,25644,95612,"0_Wed Jun 15 2022 05:13:49 GMT+0800","2022-05-22T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","IGG firing but having flame failure alarm, flame eye requested, suspect the control valves now, still not succeeded.","E/R - Aux. Mach.","Cargo / Ballast Systems","Equipment Related","10.32","Very High","","","IGG FLAME EYE RENWED TRIED OUT , FOUND SATISFACTORY.","2022-09-21T23:59:09.999","SSUN220098","Completed","2022-09-21T23:59:09.999","No","No","No","Internal"]
[null,null,null,25828,97126,"55_Thu Jun 23 2022 19:59:40 GMT+0800","2022-05-27T23:59:09.999","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Manhole covers on deck to de rust especially areas near the tightening nuts.","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.3","Medium","","","De rusting / painting of Manhole covers on deck  Completed","2022-08-27T23:59:09.999","","Completed","2022-08-07T23:59:09.999","No","No","No","Internal"]
[null,null,null,25829,83555,"55_Thu Jun 23 2022 20:31:42 GMT+0800","2022-05-27T23:59:09.999","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Spot rust and weeping marks observed on Slop P & S Steam manifold.","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.3","Medium","","","De rusting and painting  carried out at Slop P & S Steam manifold.","2022-06-26T23:59:09.999","","Completed","2022-06-11T23:59:09.999","No","No","No","Internal"]
[null,null,null,25830,74907,"55_Thu Jun 23 2022 21:01:20 GMT+0800","2022-05-27T23:59:09.999","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Spot rust and weeping marks observed on COT, WBT Tank domes and Hydraulic valve boxes especially near the Butterfly nuts.","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.3","Medium","","","Spot rust and weeping marks observed on COT, WBT Tank domes and Hydraulic valve boxes especially near the Butterfly nuts completed , ","2022-08-27T23:59:09.999","","Completed","2022-08-07T23:59:09.999","No","No","No","Internal"]
[null,null,null,25831,86922,"55_Thu Jun 23 2022 21:27:26 GMT+0800","2022-05-27T23:59:09.999","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Spot rust and weeping marks observed on Deck pipelines near the supports, U Clamps and flanges.","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.4","Very High","","","Spot de rusting and painting on deck pipelines near the supports, U Clamps and flanges completed","2022-08-27T23:59:09.999","","Completed","2022-08-20T23:59:09.999","No","No","No","Internal"]
[null,null,null,25832,16683,"55_Thu Jun 23 2022 19:14:14 GMT+0800","2022-05-27T23:59:09.999","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","SWL not marked on pad eye in Pump room .","Deck - Pipe / Fittings","General Appearance","Human Error","8.50","Medium","","","SWL marked on pad eyes in pump room.","2022-06-11T23:59:09.999","","Completed","2022-06-02T23:59:09.999","No","No","No","Internal"]
[null,null,null,25833,62282,"55_Thu Jun 23 2022 19:20:58 GMT+0800","2022-05-27T23:59:09.999","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","1 no Garbage bin in Hospital and 1 no in Crew Messroom is not color coded as per Garbage management plan ","Accommodation","General Appearance","Human Error","6.20","Medium","","","Garbage bin in Hospital and Crew Messroom color coded and labelled as per Garbage management plan.","2022-06-11T23:59:09.999","","Completed","2022-05-30T23:59:09.999","No","No","No","Internal"]
[null,null,null,25834,35875,"55_Thu Jun 23 2022 19:25:47 GMT+0800","2022-05-27T23:59:09.999","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Cleaning equipment’s kept in pipe and duct space to remove.","Accommodation","General Appearance","Human Error","11.8","Low","","","Removed cleaning equipment, which kept in pipe and duct space and Notice posted.","2022-06-02T23:59:09.999","","Completed","2022-05-30T23:59:09.999","No","No","No","Internal"]
[null,null,null,25835,47274,"55_Thu Jun 23 2022 19:30:52 GMT+0800","2022-05-27T23:59:09.999","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","All Duty officers to be familiarized with the BWTS and procedures to be posted.","Documentation","Cargo / Ballast Systems","Human Error","6.21","High","","","Familiarisation carried out  regarding BWTS procedure and same has been posted in CCR.","2022-06-11T23:59:09.999","","Completed","2022-05-31T23:59:09.999","No","No","No","Internal"]
[null,null,null,25836,34729,"55_Thu Jun 23 2022 19:35:45 GMT+0800","2022-05-27T23:59:09.999","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Locking pin for Lifebuoys on Deck to be checked for free movement as some of them are painted over.","LSA / FFA","Safety / LSA / FFA","Human Error","5.31","High","","","De rusting and painting of Locking pin of life buoys carried out.\nConfirmed free movement of the same.\n","2022-06-03T23:59:09.999","","Completed","2022-06-02T23:59:09.999","No","No","No","Internal"]
[null,null,null,25837,31362,"55_Thu Jun 23 2022 19:52:11 GMT+0800","2022-05-27T23:59:09.999","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Spare Vapor manifold reducers kept in Midship stores to check for compliance with requirements of OCIMF.","Deck - Machinery","Cargo / Ballast Systems","Equipment Related","8.42","Medium","","","12’ o clock stud pcs were missing for spare vapor manifold reducer.\nNew stud pcs fabricated for the same as per OCIMF requirement. \n","2022-06-11T23:59:09.999","","Completed","2022-06-01T23:59:09.999","No","No","No","Internal"]
[null,null,null,25838,46331,"55_Thu Jun 23 2022 20:39:26 GMT+0800","2022-05-27T23:59:09.999","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","All PV Valves vacuum side wire mesh having Rust spots and stains.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.21","High","","","PV valve vacuum side wire mesh renewed with new wire mesh. ","2022-06-26T23:59:09.999","","Completed","2022-06-02T23:59:09.999","No","No","No","Internal"]
[null,null,null,25839,18806,"55_Fri Jun 24 2022 00:30:38 GMT+0800","2022-05-27T23:59:09.999","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","All lifting gears on Deck to be tagged and marked as per the inventory.","Deck - Machinery","General Appearance","Human Error","8.50","Medium","","","Lifting gear tagged as per the inventory.","2022-06-16T23:59:09.999","","Completed","2022-06-02T23:59:09.999","No","No","No","Internal"]
[null,null,null,25840,64245,"55_Fri Jun 24 2022 00:45:50 GMT+0800","2022-05-27T23:59:09.999","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","No wire lashing for Heavy equipment and stores in Port midship store.","Deck - Machinery","General Appearance","Human Error","5.11","Low","","","Wire lashing taken for heavy equipment in Port midship store.","2022-06-11T23:59:09.999","","Completed","2022-06-01T23:59:09.999","No","No","No","Internal"]
[null,null,null,25841,70941,"55_Thu Jun 23 2022 19:08:43 GMT+0800","2022-05-27T23:59:09.999","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Railing near WBP 2 on bottom platform in Pump room not secured (Bolts loose and some missing).","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","Equipment Related","5.11","Low","","","Railing near WBP 2 on bottom platform in Pump room secured with Bolts and nuts & tighten.","2022-06-11T23:59:09.999","","Completed","2022-05-30T23:59:09.999","No","No","No","Internal"]
[null,null,null,25842,17680,"55_Fri Jun 24 2022 00:50:26 GMT+0800","2022-05-27T23:59:09.999","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Max stowage line for Sprinkler not marked in Sample locker.","LSA / FFA","Safety / LSA / FFA","Human Error","5.48","Medium","","","Max stowage line for Sprinkler marked in Sample locker.","2022-06-11T23:59:09.999","","Completed","2022-06-02T23:59:09.999","No","No","No","Internal"]
[null,null,null,25843,36644,"55_Fri Jun 24 2022 18:34:08 GMT+0800","2022-05-27T23:59:09.999","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","2 nos Safety harness in Stbd midship store in poor condition.","LSA / FFA","Safety / LSA / FFA","Human Error","5.5","Low","","","2 Safety harness kept in stbd mid ship store were not in use, same has been removed from stbd midship store and discarded. Safety harness with two lanyard, two snap hooks and an energy absorber kept in mid ship store.","2022-06-03T23:59:09.999","","Completed","2022-05-31T23:59:09.999","No","No","No","Internal"]
[null,null,null,26355,73012,"55_Tue Jul 12 2022 02:26:34 GMT+0800","2022-05-27T23:59:09.999","Observation","Ship Staff","Ship Staff Insp.","Bridge wing control console speed log repeater not readable with max brilliance in the day light time.","Navigation - Echo Sounder / Speed Log","Navigation","Equipment Related","","","","","After cleaning contactors of cables and restarting Bridge wing control console speed log repeater panel clearly visible","2022-10-12T23:59:09.999","","Completed","2022-07-13T23:59:09.999","No","No","No","Internal"]
[null,null,null,25844,33742,"55_Fri Jun 24 2022 00:00:04 GMT+0800","2022-05-27T23:59:09.999","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","All portable ladders on Deck not tagged and inventory not maintained.","Deck - Machinery","General Appearance","Human Error","8.50","Medium","","","All portable ladders on Deck tagged and inventory maintained for the same","2022-06-16T23:59:09.999","","Completed","2022-06-05T23:59:09.999","No","No","No","Internal"]
[null,null,null,25845,83648,"55_Thu Jun 23 2022 19:42:03 GMT+0800","2022-05-27T23:59:09.999","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Locking pin for Hook of Stbd davit in Sunken deck and Bosun store davit is frozen.","Deck - Machinery","Safety / LSA / FFA","Equipment Related","8.50","Medium","","","Locking pin for Hook of Stbd davit in Sunken deck and Bosun store davit greased and confirmed free movement.","2022-06-11T23:59:09.999","","Completed","2022-06-05T23:59:09.999","No","No","No","Internal"]
[null,null,null,25847,12387,"55_Fri Jun 24 2022 18:46:13 GMT+0800","2022-05-27T23:59:09.999","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Bilge cover for Aft Bilge well near Propeller shaft on port side is missing.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Human Error","10.15","Low","","","Bilge cover for Aft Bilge well near Propeller shaft to be put back in position.","2022-06-16T23:59:09.999","","Completed","2022-06-01T23:59:09.999","No","No","No","Internal"]
[null,null,null,25848,27902,"55_Fri Jun 24 2022 18:51:21 GMT+0800","2022-05-27T23:59:09.999","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Max stowage line for Sprinkler not marked in Chemical locker.","LSA / FFA","Safety / LSA / FFA","Human Error","5.48","Medium","","","Max stowage line for Sprinkler to be marked in Chemical locker.","2022-06-11T23:59:09.999","","Completed","2022-06-02T23:59:09.999","No","No","No","Internal"]
[null,null,null,26503,33172,"55_Sun Aug 14 2022 19:29:02 GMT+0800","2022-07-18T23:59:09.999","Observation","Ship Staff","Ship Staff Insp.","WHRS BELLOW AT LP SECTION PORT SIDE HOLED","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","BLAST FURNANCE CEMENT APPLIED ON HOLE","2022-10-17T23:59:09.999","","Completed","2022-09-02T23:59:09.999","No","No","No","Internal"]
[null,null,null,26647,22681,"55_Wed Aug 31 2022 18:05:11 GMT+0800","2022-08-04T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","It was observed that the Loadicator display was not coming. The CPU was restarted and it was observed that there is no output signal to the display ,also that the CPU processor fan upon restarting was cutting in and off continuously & no output through the terminal ports  .Suspect motherboard malfunction  .","Miscellaneous","Cargo / Ballast Systems","Equipment Related","9.7","Medium","","","Received new CPU with preloaded loadicator software ","2022-09-18T23:59:09.999","","Completed","2022-09-16T23:59:09.999","No","No","No","Internal"]
[null,null,null,26646,46817,"55_Wed Aug 31 2022 17:58:20 GMT+0800","2022-08-12T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","STBD WINDLASS SPLIT DRUM BUSH HAS BEEN DISLOCATED FROM PLACE CAUSING UNDUE NOISE AND WOBBLE OF SPLIT DRUM.","Deck - Machinery","Mooring","Equipment Related","9.14","Medium","","","Sleeve bearing of stbd windlass drum renewed.","2023-02-19T23:59:09.999","SSUN220193","Completed","2023-02-10T23:59:09.999","No","No","No","Internal"]
[null,null,null,26780,36264,"55_Tue Sep 13 2022 16:19:07 GMT+0800","2022-08-15T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","16K/8.5K Steam Control Valve Positioner does not feed back values to AMS ","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","11.10","Medium","","","New spare positioner received & replaced","2022-11-14T23:59:09.999","SSUN220192","Completed","2022-11-03T23:59:09.999","No","No","No","Internal"]
[null,null,null,26785,75506,"55_Wed Sep 14 2022 16:30:35 GMT+0800","2022-08-15T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","Auto-Telephone for bridge, CO2 room, elevator machinery room was not operational due faulty unit and PCB","Elect. Mach. & Equip.","Communication","Equipment Related","10.11","Medium","","","ALL MENTIONED TELEPHONES MADE OPERATIONAL","2022-11-14T23:59:09.999","SSUN220194\nSSUN220111","Completed","2022-09-21T23:59:09.999","No","No","No","Internal"]
[null,null,null,26786,42025,"55_Thu Sep 15 2022 17:45:32 GMT+0800","2022-08-16T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","VISCOSENSOR VALVE PASSING, NO MAINTENANCE CAN BE CARRIED OUT ON VISCOSENSOR.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","VESSEL TO DO MAINTENANCE WHILE ON MGO.\nVALVES TO BE ORSERED IN NEXT BUDGET","2022-11-15T23:59:09.999","SSUN220189","Completed","2022-09-15T23:59:09.999","No","No","No","Internal"]
[null,null,null,26787,63197,"55_Thu Sep 15 2022 17:43:34 GMT+0800","2022-08-16T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","MAIN COPT/CSW PUMP DISCHARGE VALVE HAS DAMAGED SLEEVE CAUSING NRV VALVE NOT FUNCTIONING AND PUMP ROTATING ANTICLOCKWISE\n","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","EXISTING VALVE GUIDE REBULIT AND PUT IN PLACE SAME WORKING GOOD.","2022-11-15T23:59:09.999","","Completed","2022-10-02T23:59:09.999","No","No","No","Internal"]
[null,null,null,26779,25214,"55_Mon Sep 12 2022 16:54:21 GMT+0800","2022-08-19T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","CONTROL AIR DRYER #1 COMPRESSOR IS HAVING FAULTY TEMP SENSOR FOR COMPRESSOR","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","NEW COMPRESSOR INSTALLED , UNIT WORKING IN GOOD CONDITION.","2022-11-18T23:59:09.999","SSUN220209","Completed","2022-09-24T23:59:09.999","No","No","No","Internal"]
[null,null,null,26777,41981,"55_Wed Sep 07 2022 21:47:08 GMT+0800","2022-08-21T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","#2 COPT Over speed relay malfunction, causing the turbine to trip at 50 to 100 rpm","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","10.32","Very High","","","Replaced with new spare received Singapore Transit","2022-11-13T23:59:09.999","SSUN220201","Completed","2022-11-04T23:59:09.999","No","No","No","Internal"]
[null,null,null,26781,25126,"55_Tue Sep 13 2022 16:35:00 GMT+0800","2022-08-22T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","Manifold pressure transmitter printer drive unit faulty","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.41","Medium","","","Renewed printer drive unit.","2022-11-21T23:59:09.999","SSUN220208","Completed","2022-11-05T23:59:09.999","No","No","No","Internal"]
[null,null,null,26782,15461,"55_Tue Sep 13 2022 17:36:26 GMT+0800","2022-08-22T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","Ballast Tank VRCS valve indicator unit transmitter value was fluctuating","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","Required spare,\nSPARES RECEIVED and job completed","2023-01-20T23:59:09.999","SSUN220204","Completed","2022-12-30T23:59:09.999","No","No","No","Internal"]
[null,null,null,26784,41234,"55_Wed Sep 14 2022 16:23:30 GMT+0800","2022-08-27T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","While trying out Anemometer alarms, only visual alarm was working, horn was not operational and the unit was also giving ESB 220 VAC Low Insulation alarm","Elect. Mach. & Equip.","Communication","Equipment Related","5.9","Very High","","","Spares received-Job completed","2022-11-26T23:59:09.999","SSUN220220","Completed","2022-11-12T23:59:09.999","No","No","No","Internal"]
[null,null,null,27153,12242,"55_Wed Sep 21 2022 09:42:16 GMT+0800","2022-08-28T23:59:09.999","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Stbd windlass operating lever hydraulic block, found leaking","Deck - Machinery","Mooring","Equipment Related","9.14","Medium","","","job completed with onboard spares RO raised to maintain ROB","2022-11-15T23:59:09.999","SSUN220118","Completed","2022-10-20T23:59:09.999","No","No","No","Internal"]
[null,null,null,27162,31454,"55_Wed Sep 21 2022 10:25:54 GMT+0800","2022-08-28T23:59:09.999","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Magnetic compass dimmer AC dimmer switch not operational.","Navigation - Others","Navigation","Equipment Related","4.7","High","","","Vessel rcvd spares at Singapore on 10th Nov 2022.  Same has been renewed.\nMagnetic compass dimmer AC dimmer switch is operational now.","2022-11-20T23:59:09.999","SSUN220184","Completed","2022-11-02T23:59:09.999","No","No","No","Internal"]
[null,null,null,27163,58309,"55_Fri Sep 23 2022 15:21:44 GMT+0800","2022-08-28T23:59:09.999","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Pressure gauge from central cooler blackened, glycerin needs renewal","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Same renewed","2022-09-08T23:59:09.999","","Completed","2022-08-25T23:59:09.999","No","No","No","Internal"]
[null,null,null,27164,44385,"55_Fri Sep 23 2022 15:25:11 GMT+0800","2022-08-28T23:59:09.999","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Missing Limit switch valve plate for APT valves","E/R - Pumps","Eng. / Strg. Comp.","Industry Issue","","","","","Plates fabricated and installed in place","2022-11-24T23:59:09.999","","Completed","2022-08-27T23:59:09.999","No","No","No","Internal"]
[null,null,null,27165,30876,"55_Wed Sep 21 2022 09:49:15 GMT+0800","2022-08-28T23:59:09.999","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Main deck port & stbd side aft of manifold area to be de rusted","Deck - Pipe / Fittings","General Appearance","External Factors","11.3","Medium","","","Main deck port and stbd side spot chipping / painting completed","2022-10-06T23:59:09.999","","Completed","2022-09-13T23:59:09.999","No","No","No","Internal"]
[null,null,null,27166,12508,"55_Wed Sep 21 2022 10:14:26 GMT+0800","2022-08-28T23:59:09.999","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Main deck cargo pipelines and associated valves in front of pumproom entry bulkhead de rusting / spot painting required.","Deck - Pipe / Fittings","General Appearance","External Factors","11.4","Very High","","","Main deck cargo pipelines and associated valves in front of pumproom entry bulkhead de rusted and spot painting carried out","2022-09-21T23:59:09.999","","Completed","2022-08-26T23:59:09.999","No","No","No","Internal"]
[null,null,null,27167,83173,"55_Wed Sep 21 2022 10:18:32 GMT+0800","2022-08-28T23:59:09.999","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Deck fixed foam system line drain in foam room was found having minor leak, drain valve to be renewed or overhauled and fixed back.","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.35","Medium","","","Deck fixed foam system line drain in foam room will be overhauled","2022-08-28T23:59:09.999","","Completed",null,"No","No","No","Internal"]
[null,null,null,27168,69229,"55_Wed Sep 21 2022 09:47:29 GMT+0800","2022-08-28T23:59:09.999","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Pumproom entrance weather tight door stbd side rubber packing to be renewed","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.6","Medium","","","Rubber packing of stbd side pumproom entrance door adjusted properly and is properly sitting in watertight groove of weather tight door","2022-09-21T23:59:09.999","","Completed","2022-09-09T23:59:09.999","No","No","No","Internal"]
[null,null,null,27170,16722,"55_Wed Sep 21 2022 09:52:04 GMT+0800","2022-08-28T23:59:09.999","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Shackles used for Anchor lashings were found having less SWL (4 Tones)  than required, as the Anchors are weighing 17.25 tones.","Deck - Mooring Machinery","Mooring","External Factors","9.2","Very High","","","Anchor lashing shackles replaced with appropriate size shackles of 17 tons","2022-10-05T23:59:09.999","SSUN-220168 – DECK STORES","Completed","2022-09-17T23:59:09.999","No","No","No","Internal"]
[null,null,null,27177,11450,"55_Wed Sep 21 2022 10:08:21 GMT+0800","2022-08-28T23:59:09.999","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Vessel does not have wire slings/shackles of appropriate SWL for testing the hose handling crane to required Load using the Load Cell.","","Cargo / Ballast Systems","Equipment Related","8.5","Very High","","","Load testing of both midship cranes carried out .Both midship cranes load tested to 20 Tons using load cell","2022-10-05T23:59:09.999","SUN-220168 – DECK STORES","Completed","2022-09-24T23:59:09.999","No","No","No","Internal"]
[null,null,null,27178,85901,"55_Fri Sep 23 2022 15:27:55 GMT+0800","2022-08-28T23:59:09.999","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Soft patch found on aft hydraulic inlet water line.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.31","Very High","","","New pipe fabricated and installed in place","2022-09-14T23:59:09.999","","Completed","2022-09-06T23:59:09.999","No","No","No","Internal"]
[null,null,null,27179,63124,"55_Wed Sep 21 2022 10:16:33 GMT+0800","2022-08-28T23:59:09.999","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Stbd Lifeboat Self-Lowering remote control wire roller sheave blocks were found having slight chaffing and same needs to be renewed with new brass blocks.","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.28","Very High","","","Stbd side lifeboat self lowering controller wire sheaves renewed with brass sheaves","2022-10-05T23:59:09.999","SSUN220190","Completed","2022-09-25T23:59:09.999","No","No","No","Internal"]
[null,null,null,27180,39256,"55_Wed Sep 21 2022 09:44:49 GMT+0800","2022-08-28T23:59:09.999","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Helicopter landing area collapsible railings spot de rusting requiring and to be highlighted","Deck - Pipe / Fittings","General Appearance","External Factors","11.3","Medium","","","Helicopter landing area collapsible railings spot de rusting and painting / highlighting completed","2022-10-06T23:59:09.999","","Completed","2022-09-25T23:59:09.999","No","No","No","Internal"]
[null,null,null,27181,60055,"55_Wed Sep 21 2022 10:12:36 GMT+0800","2022-08-28T23:59:09.999","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Paint locker sprinkler system drain valve leaking same to be overhauled.","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.35","Medium","","","Paint locker sprinkler system drain valve overhauled","2022-09-14T23:59:09.999","","Completed","2022-08-23T23:59:09.999","No","No","No","Internal"]
[null,null,null,27182,35572,"55_Wed Sep 21 2022 10:23:52 GMT+0800","2022-08-28T23:59:09.999","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Course recorder marking / printing observed faded during routine inspection. Spare set of Stylus has been ordered. Stylus adjusted presently.","Navigation - Others","Navigation","Equipment Related","4.7","High","","","Course recorder stylus replaced with new one . Working satisfactorily","2022-11-20T23:59:09.999","SSUN220152","Completed","2022-09-19T23:59:09.999","No","No","No","Internal"]
[null,null,null,27156,80155,"55_Sun Oct 02 2022 10:41:14 GMT+0800","2022-09-14T23:59:09.999","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","EGCS JET SECTION SW INLET PIPE STUB PIECE TO BE RENEWED","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","VESSEL AWAITNG SPARES, PRESENTLY REMOVED PIPE AND BUILD UP FOR THE HOLED SECTION HAS BEEN CARRIED OUT, SAME PRESSURE TESTED AND PUT IN USE AND PRESNETLY NOT LEAKING .","2023-01-14T23:59:09.999","SSUN220216","Completed","2022-12-24T23:59:09.999","No","No","No","Internal"]
[null,null,null,27157,10918,"55_Sun Oct 02 2022 10:53:16 GMT+0800","2022-09-14T23:59:09.999","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","HP drum safety valve to be renewed. Spare safety valve supplied to vessel.","E/R - Boiler","Eng. / Strg. Comp.","External Factors","10.32","Very High","","","HP DRUM SV HAS PITTING ON VALVE SEAT SAME WILL BE RENEWED AT NEXT AVALABLE OPPURTUNITY..","2022-12-14T23:59:09.999","","Completed","2022-10-04T23:59:09.999","No","No","No","Internal"]
[null,null,null,27158,54326,"55_Sun Oct 02 2022 10:54:20 GMT+0800","2022-09-14T23:59:09.999","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Sludge collecting tank steam heating valve leaking. Same to be renewed","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Valve to be renewed once vessel changes over to MGO .\n","2022-12-14T23:59:09.999","","Completed","2022-10-03T23:59:09.999","No","No","No","Internal"]
[null,null,null,27159,85971,"55_Sun Oct 02 2022 10:52:01 GMT+0800","2022-09-14T23:59:09.999","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Funnel deck floor need chipping and painting. Special paint supplied for this to be used.","Miscellaneous","General Appearance","Equipment Related","11.1","High","","","Funnel deck chipped and re painted.","2023-01-14T23:59:09.999","","Completed","2023-01-03T23:59:09.999","No","No","No","Internal"]
[null,null,null,27160,27267,"55_Sun Oct 02 2022 10:56:09 GMT+0800","2022-09-14T23:59:09.999","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Work shop fire door is bent. Same need renewal.","LSA / FFA","Eng. / Strg. Comp.","Equipment Related","5.14","Very High","","","Replaced with new one","2023-01-14T23:59:09.999","","Completed","2022-11-15T23:59:09.999","No","No","No","Internal"]
[null,null,null,27169,27494,"55_Sun Oct 02 2022 10:50:01 GMT+0800","2022-09-14T23:59:09.999","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","NO.3 ER FAN ROOM CEILING NEEDS REPAIR","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","CEILING HAS FALLEN DOWN FROM SUPPORT. NEW SUPPORT TO BE FABRICATED AND CEILING TO BE SECURED.","2022-12-14T23:59:09.999","","Completed","2022-09-18T23:59:09.999","No","No","No","Internal"]
[null,null,null,27171,68393,"55_Sun Oct 02 2022 10:57:18 GMT+0800","2022-09-14T23:59:09.999","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","S/G bilge drain valve frozen. Same to be overhauled and eased up.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Valve to be dismantled and overhauled.","2022-10-14T23:59:09.999","","Completed","2022-09-19T23:59:09.999","No","No","No","Internal"]
[null,null,null,27172,77168,"55_Sun Oct 02 2022 10:44:05 GMT+0800","2022-09-14T23:59:09.999","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","EGCS DECK HOUSE NEEDS CLEANING","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","CLEANING DONE, PAINTING WILL BE CARRIED OUT PRIOR ARRIVAL PORT","2022-10-14T23:59:09.999","","Completed","2022-09-18T23:59:09.999","No","No","No","Internal"]
[null,null,null,27173,42401,"55_Sun Oct 02 2022 10:47:45 GMT+0800","2022-09-14T23:59:09.999","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","MIST CATCHER IN ER HAS OIL LEAKAGE MARKS. TO BE OPENED AND INSPECTED.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","FLANGES RE TIGHTENED ","2022-10-14T23:59:09.999","","Completed","2022-09-18T23:59:09.999","No","No","No","Internal"]
[null,null,null,27174,26780,"55_Sun Oct 02 2022 10:58:03 GMT+0800","2022-09-14T23:59:09.999","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","EFP room bilge drain valve frozen. Same to be overhauled and eased up.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Valve to be overhauled","2022-10-14T23:59:09.999","","Completed","2022-09-19T23:59:09.999","No","No","No","Internal"]
[null,null,null,27175,84071,"55_Sun Oct 02 2022 08:40:53 GMT+0800","2022-09-14T23:59:09.999","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Port Windlass brake cylinder match marks not aligned. To be adjusted as per maker’s manual procedure. Match marks on both windlass to be highlighted.","Deck - Mooring Machinery","Mooring","Equipment Related","9.20","Medium","","","Port Windlass brake cylinder match marks  aligned and  adjusted as per maker’s manual procedure. Match marks on both windlass highlighted.","2022-11-13T23:59:09.999","","Completed","2022-09-22T23:59:09.999","No","No","No","Internal"]
[null,null,null,27176,32584,"55_Sun Oct 02 2022 08:45:21 GMT+0800","2022-09-14T23:59:09.999","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Port Windlass gear oil to renew.","Deck - Mooring Machinery","Mooring","Equipment Related","9.14","Medium","","","Port Windlass gear oil renewed","2022-10-14T23:59:09.999","","Completed","2022-09-24T23:59:09.999","No","No","No","Internal"]
[null,null,null,27360,76799,"55_Tue Oct 18 2022 20:05:01 GMT+0800","2022-10-03T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","SHIP'S LAUNDRY WASHING MACHINE NOT OPERATIONAL","Accommodation","MLC Related","Equipment Related","","","","","NEW WASHING MACHINE RECEIVED. JOB COMPLETED","2022-11-15T23:59:09.999","SSUN220245","Completed","2022-11-15T23:59:09.999","No","No","No","Internal"]
[null,null,null,29385,54697,"55_Thu Mar 16 2023 00:00:33 GMT+0800","2022-10-05T23:59:09.999","Non Conformity","Ship Staff","Nav Audit / Verification","Position Plotting Intervals in Singapore Strait was not followed as per ENC Marking.","Navigation - ECDIS","Navigation","Human Error","","","","","All OOWs briefed on the requirements of position verification intervals with instructions / requirements. ","2023-01-04T23:59:09.999","","Completed","2022-10-31T23:59:09.999","No","No","No","Internal"]
[null,null,null,29386,12842,"55_Thu Mar 16 2023 00:03:14 GMT+0800","2022-10-05T23:59:09.999","Non Conformity","Ship Staff","Nav Audit / Verification","Steering Light was found In-operational during Audit Checks. ","Navigation - Others","Navigation","Human Error","","","","","Faulty Steering light fixture replaced with new spare and tried out found working satisfactory.","2023-01-04T23:59:09.999","","Completed","2022-10-09T23:59:09.999","No","No","No","Internal","Please discuss this observation and preventive action in next safety meeting/tool box meeting, with the officers/crew involved, to avoid recurrence."]
[null,null,null,29387,19252,"55_Thu Mar 16 2023 00:06:42 GMT+0800","2022-10-05T23:59:09.999","Non Conformity","Ship Staff","Nav Audit / Verification","Historical Records checked and found that Draft entries from last Disport to Singapore in Deck Log Book was not there. ","Navigation - Others","Navigation","Human Error","","","","","Relevant draft entries made in the deck log books by new bridge team officers and All OOWs briefed about making entries in bridge bell book and deck log books in line with instructions / requirements on regular basis.","2022-10-31T23:59:09.999","","Completed","2022-10-31T23:59:09.999","No","No","No","Internal","Please discuss this observation and preventive action in next safety meeting/tool box meeting, with the officers/crew involved, to avoid recurrence."]
[null,null,null,27365,99234,"55_Mon Oct 31 2022 15:45:21 GMT+0800","2022-10-08T23:59:09.999","Observation","Ship Staff","Ship Staff Insp.","BRIDGE AIR CON BLOWER WOBBLING","Miscellaneous","MLC Related","Equipment Related","","","","","Fan belt replaced and now no wobbling. noticed pulley wheel to have crack same shall be requested from vessel end.","2023-01-07T23:59:09.999","","Completed","2022-12-23T23:59:09.999","No","No","No","Internal"]
[null,null,null,27364,29748,"55_Mon Oct 31 2022 15:46:58 GMT+0800","2022-10-14T23:59:09.999","Observation","Ship Staff","Ship Staff Insp.","ER BLOWERS ON DECK HAS RUST ON BASE AND HINGES","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","Equipment Related","11.4","Very High","","","DE RUSTING  AND PAINTING CARIED OUT.","2022-11-18T23:59:09.999","","Completed","2022-11-17T23:59:09.999","No","No","No","Internal"]
[null,null,null,27362,25555,"55_Tue Oct 25 2022 15:00:40 GMT+0800","2022-10-20T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","EGCS SCRUBBER PUMP VFD PANEL B PORTABLE AC NOT WORKING DUE TO BURNT PCB FOR DISPLAY","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","Spare received, replaced and rectified.","2023-02-20T23:59:09.999","","Completed","2023-02-19T23:59:09.999","No","No","No","Internal","RO no not mentioned in the PO Ref no."]
[null,null,null,27363,17261,"55_Tue Oct 25 2022 14:58:51 GMT+0800","2022-10-20T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","WHRS EXHAUST OUTLET SENSOR NO.21 NOT WORKING AND GIVING SENSOR FAIL ALARM","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","WHRS exhaust outlet faulty sensor No. 21 replaced with new, which was received during last call at Singapore","2023-08-14T23:59:09.999","","Completed","2023-08-05T23:59:09.999","No","No","No","Internal",""]
[null,null,null,27155,63938,"55_Sun Oct 02 2022 08:48:05 GMT+0800","2022-10-21T23:59:09.999","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","VRCS piping on deck need de-rusting and painting.","Deck - Pipe / Fittings","General Appearance","External Factors","11.4","Very High","","","VRCS Line Derusting and Painting Completed\n","2023-07-31T23:59:09.999","","Completed","2023-06-07T23:59:09.999","No","No","No","Internal"]
[null,null,null,27154,70816,"55_Wed Sep 21 2022 10:10:43 GMT+0800","2022-10-24T23:59:09.999","Other","Owner / Marine / Tech. Suptd.","Ship Staff Insp.","Accommodation superstructure deck spot de rusting / painting required.","Accommodation","General Appearance","External Factors","11.8","Low","","","Work Aloft on Accommodation Block and Funnel Casing Completed at Anchorage during Port Stay at Cap Lopez, Gabon. All accessible spots in Accommodation Front, Sides, Bridge Wing, Bulwark Supporting Bridge Wing spot de-rusted, primer and final coat completed. ","2023-08-30T23:59:09.999","","Completed","2023-03-22T23:59:09.999","No","No","No","Internal"]
[null,null,null,27361,89196,"55_Thu Oct 20 2022 13:53:35 GMT+0800","2022-10-27T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","E/R OIL  MIST DETECTOR FOR PURIFIER ROOM FAULTY","LSA / FFA","Eng. / Strg. Comp.","Equipment Related","","","","","SPARES RECEIVED FAULTY DETECTOR REPLACED, WORKING SATISFACTORY.","2023-06-27T23:59:09.999","SSUN230014","Completed","2023-06-07T23:59:09.999","No","No","No","Internal","Spares will be supplied at next available opportunity."]
[null,null,null,26357,81857,"55_Mon Aug 01 2022 19:45:51 GMT+0800","2022-11-01T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","MAIN ENGINE STBD BRIDGE WING CONSOLE OUT OF ORDER DUE TO BWU09 MODULE NOT OPERATIONAL","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.31","Very High","","","Kongsberg engineer attended all put back to normal . No alarm since singapore.","2023-02-18T23:59:09.999","","Completed","2023-02-20T23:59:09.999","No","No","No","Internal","Servicing will be arranged next call Singapore."]
[null,null,null,27161,15694,"55_Tue Oct 04 2022 10:10:35 GMT+0800","2022-11-11T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","Loadicator unale to activate online data from rosemount tank gauging online feed system","Miscellaneous","Cargo / Ballast Systems","Equipment Related","9.7","Medium","","","Troubleshooting in progress , office advised regarding the same\nEmerson Technician attended at Singapore on 21 Feb 23, reported, NAPA Technician remote assistance provided and the job is completed now","2023-04-23T23:59:09.999","","Completed","2023-03-20T23:59:09.999","No","No","No","Internal"]
[null,null,null,27959,96099,"55_Fri Dec 16 2022 06:54:21 GMT+0800","2022-11-13T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","Fwd Catwalk platform got deformed & buckled, also railing of the same platform bent towards outer side, due to heavy weather impact. ","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.3","Medium","","","Straightening of deformed Fwd Catwalk platform and railing done.\n","2022-12-19T23:59:09.999","","Completed","2022-11-20T23:59:09.999","No","No","No","Internal"]
[null,null,null,26504,81077,"55_Sun Aug 14 2022 19:39:40 GMT+0800","2022-11-14T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","Signal Column at E/R bottom platform . FWD. STBD. not working. Found transformer burnt for same","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","New spare received -PCB-replaced-system unit made operational-tested","2023-07-29T23:59:09.999","SSUN230019","Completed","2023-07-24T23:59:09.999","No","No","No","Internal"]
[null,null,null,25638,29484,"55_Wed Jun 15 2022 02:36:41 GMT+0800","2022-11-16T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","CLO pump worn off alarm is appearing while running ICO lube.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Both Stator of System oil and cylinder oil pump renewed with spare received. System tried out and all found satisfactory. \n","2024-02-01T23:59:09.999","SSUN230009","Completed","2023-12-15T23:59:09.999","No","No","No","Internal",""]
[null,null,null,27956,96804,"55_Fri Dec 16 2022 06:27:01 GMT+0800","2022-11-20T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","Support bracket for ME Fuel Supply unit Inlet & Outlet pipe manifold has a crack","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","SUPPORT BRACKET WELDING JOB COMPLETED AFTER OFFICE CONCURRENCE.","2023-04-19T23:59:09.999","","Completed","2023-04-05T23:59:09.999","No","No","No","Internal"]
[null,null,null,null,31172,"55_Sat Apr 12 2025 00:28:25 GMT+0800","2025-02-13T08:00:00","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Sea Water leaks on the FWG to be rectified.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","leak rectified and system tried out, found satisfactory.","2025-05-13T08:00:00","","Completed","2025-05-01T08:00:00","No","No","No","Internal","Identify the leaks and rectify."]
[null,null,null,27955,36927,"55_Fri Dec 16 2022 03:41:59 GMT+0800","2022-11-28T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","Following COW machine valves were found passing during pressure testing of COW line prior discharge port.\n2P(1 Nos),  2S (1Nos), 3S (1Nos), 4P(1Nos), 1C(2Nos)","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.34","High","","","COW Machine valves Seat Rings renewed. \nWill be rechecked during line pressure testing. ","2023-05-26T23:59:09.999","SSUN230053.","Completed","2023-03-13T23:59:09.999","No","No","No","Internal"]
[null,null,null,27958,36802,"55_Fri Dec 16 2022 03:14:29 GMT+0800","2022-12-01T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","No.1 & No.2 Foam monitor valve is leaking.","LSA / FFA","Emgcy. Systems","Equipment Related","5.38","High","","","No.2  and No.1 Foam monitor valve replaced, Foam monitor tested, no leak detected.\n","2022-12-18T23:59:09.999","","Completed","2022-12-03T23:59:09.999","No","No","No","Internal"]
[null,null,null,27953,68643,"55_Fri Dec 16 2022 03:19:45 GMT+0800","2022-12-03T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","No.3 and No.2 Fire line Isolation valve is leaking.","LSA / FFA","Emgcy. Systems","Equipment Related","5.38","High","","","Isolation valves overhauled. Isolation valves tested after overhauling, found in order.","2022-12-18T23:59:09.999","","Completed","2022-12-17T23:59:09.999","No","No","No","Internal"]
[null,null,null,27954,56662,"55_Fri Dec 16 2022 03:24:36 GMT+0800","2022-12-03T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","Valve between IG line to VECS line cannot be closed properly, presently valve is in open condition and will not cause any problem for discharging operation.","Inert Gas","Cargo / Ballast Systems","Equipment Related","8.30","High","","","Fabricated new key for valve stem and put back the mechanical actuator in position & confirmed valve is opening and shutting properly. \nValve were removed to checked for opening and shutting position. Valve is opening and shutting properly. ","2023-01-20T23:59:09.999","","Completed","2022-12-29T23:59:09.999","No","No","No","Internal"]
[null,null,null,26356,45280,"55_Sat Jul 30 2022 09:01:39 GMT+0800","2022-12-05T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","VRCS UNLOADER MECHANISM NOT OPERATIONAL","Deck - Machinery","Cargo / Ballast Systems","Equipment Related","8.31","High","","","Unloader switch received at 21/02/2023 and replaced now in order.","2023-03-19T23:59:09.999","SSUN220141","Completed","2023-03-02T23:59:09.999","No","No","No","Internal"]
[null,null,null,26783,86098,"55_Tue Sep 13 2022 17:51:37 GMT+0800","2022-12-07T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","#1  Economiser Feed Water pump motor, while running observed heavy vibration and abnormal sound, also observed bearing seat was damaged","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Motor received installed tried out and in order now.","2023-03-19T23:59:09.999","SSUN220182","Completed","2023-02-16T23:59:09.999","No","No","No","Internal"]
[null,null,null,28142,53498,"0_Fri Dec 30 2022 05:57:24 GMT+0800","2022-12-10T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","NO1 CSW PUMP DISCHARGE VALVE NOT HOLDING. IT WAS INFORMED THAT VALVE PARTS WERE FOUND IN LT COOLER.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","All 3 main cooling sea water pump discharge valves leak test carried out and observed No1 cooling sea water discharge valve holding even with the discharge valve open condition (NR valve).\nHowever NO 3 Main cooling sea water pump discharge valve found not holding even with discharge valve completely shut (manually).\nVessel renewed No 3 Main cooling sea water pump discharge valve with new spare.\n","2023-11-30T23:59:09.999","SSUN230045","Completed","2023-10-13T23:59:09.999","No","No","No","Internal"]
[null,null,null,28143,97657,"55_Fri Dec 30 2022 05:50:10 GMT+0800","2022-12-10T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","HP DRUM GUAGE GLASS LEAKING","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","Guage glass of HP drum was erroded and erroded surface filled up with permatex high temperature and was fitted in place. As of now it is an temporary repair and no leaks.","2023-01-20T23:59:09.999","SSUN230029","Completed","2023-01-14T23:59:09.999","No","No","No","Internal","Believe in the mean time you can use high press gaskets."]
[null,null,null,28136,17214,"0_Fri Dec 30 2022 05:59:13 GMT+0800","2022-12-11T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","3 way valve of no1 HFO purifier found to be leaking same needs to be renewed,","E/R - Purifier","Eng. / Strg. Comp.","Equipment Related","","","","","3 Way valve for HFO purifier no.1 renewed.","2023-01-20T23:59:09.999","","Completed","2022-12-25T23:59:09.999","No","No","No","Internal"]
[null,null,null,28137,14413,"55_Fri Dec 30 2022 06:51:27 GMT+0800","2022-12-11T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","Servo oil Filter screen flashing and not readable.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","File taking inventory we found one spare display. Same replaced.","2023-03-11T23:59:09.999","","Completed","2023-01-11T23:59:09.999","No","No","No","Internal"]
[null,null,null,28138,53534,"0_Fri Dec 30 2022 06:55:50 GMT+0800","2022-12-11T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","STarboard Lifeboat batteries were renewed with old batteries as the batteries in place failed to start.","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","Battery ordered through SSUN230004 received and replaced.","2023-03-18T23:59:09.999","SSUN230004","Completed","2023-02-15T23:59:09.999","No","No","No","Internal"]
[null,null,null,28139,97293,"0_Fri Dec 30 2022 06:57:36 GMT+0800","2022-12-11T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","Vessel received UPS for CITADEL but our AMS UPS had breakdown and hence we installed CITADEL UPS to AMS.","Miscellaneous","Safety / LSA / FFA","Equipment Related","","","","","Received UPS-Battery- connected to Citadel Communication phone.","2023-09-30T23:59:09.999","SSUN230007","Completed","2023-09-15T23:59:09.999","No","No","No","Internal"]
[null,null,null,28141,83230,"0_Fri Dec 30 2022 06:53:45 GMT+0800","2022-12-11T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","Accomodation Gas detection system sensors are all expired and give alarm at times and calibration is not accepting many times.","Accommodation","Safety / LSA / FFA","Equipment Related","","","","","Sensors are already in order through SSUN23003-Last testing of alarms were satisfactory, No alarm on panel.","2023-09-15T23:59:09.999","SSUN230003","Completed","2023-09-15T23:59:09.999","No","No","No","Internal"]
[null,null,null,28360,22456,"55_Mon Jan 16 2023 06:07:58 GMT+0800","2022-12-15T23:59:09.999","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Walkway Fwd of midship not marked.","Miscellaneous","General Appearance","Inappropriate Procedure","11.8","Low","","","Painting Completed","2023-06-27T23:59:09.999","","Completed","2023-06-13T23:59:09.999","No","No","No","Internal"]
[null,null,null,28140,71489,"55_Wed Dec 28 2022 23:42:48 GMT+0800","2022-12-15T23:59:09.999","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","SOLAS TRAINING MANUALS was not made per ship Specific.","LSA / FFA","Safety / LSA / FFA","Human Error","5.15","Medium","","","* SOLAS TRAINING MANUALS to be made ship – Completed","2023-01-04T23:59:09.999","","Completed","2023-01-03T23:59:09.999","No","No","No","Internal"]
[null,null,null,28144,61013,"55_Wed Dec 28 2022 23:23:25 GMT+0800","2022-12-15T23:59:09.999","Observation","Owner / Marine / Tech. Suptd.","ISM Audit","Boiler in Pantry was not secured.","Accommodation","MLC Related","Human Error","11.13","Low","","","Boiler in Pantry secured with fixed securing arrangement.","2022-12-20T23:59:09.999","","Completed","2022-12-17T23:59:09.999","No","No","No","Internal"]
[null,null,null,28145,47746,"55_Wed Dec 28 2022 23:20:33 GMT+0800","2022-12-15T23:59:09.999","Observation","Owner / Marine / Tech. Suptd.","MLC Audit","Deep Fat Fryer in Galley was not secured.\n","Accommodation","MLC Related","Human Error","11.13","Low","","","Deep Fat Fryer in Galley secured With fixed securing arrangement..","2022-12-20T23:59:09.999","","Completed","2022-12-17T23:59:09.999","No","No","No","Internal"]
[null,null,null,28135,95809,"55_Wed Dec 28 2022 21:57:23 GMT+0800","2022-12-17T23:59:09.999","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Immersion Suit Air Pressure testing last carried out in Nov 2020, Manufactured in 2011. Annual pressure test required. Last Annual Carried out in Feb 2022 does not have records of Air Pressure test.","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.33","High","","","Immersion suits  Air Pressure tested using pressure testing kit available onboard.","2023-01-04T23:59:09.999","","Completed","2022-12-27T23:59:09.999","No","No","No","Internal"]
[null,null,null,29388,32838,"55_Thu Mar 16 2023 00:09:59 GMT+0800","2022-12-28T23:59:09.999","Observation,Non Conformity","Ship Staff","Nav Audit / Verification","During Navigational Audit found that Damage Control Plan was found missing from Emergency Plan Box on Bridge.","Navigation - Others","Navigation","Human Error","","","","","Same has been found in Bridge drawer and put back in place (Emergency Plan Box).","2023-03-27T23:59:09.999","","Completed","2022-12-28T23:59:09.999","No","No","No","Internal","Please discuss this observation and preventive action in next safety meeting/tool box meeting, with the officers/crew involved, to avoid recurrence."]
[null,null,null,28656,13559,"55_Sat Jan 21 2023 05:33:21 GMT+0800","2023-01-08T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","VECS o2 sensor is expired","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","","","","","Expired O2 sensor replaced with new one received and calibration carried out, working satisfactory.","2023-04-11T23:59:09.999","SSUN230044","Completed","2023-04-20T23:59:09.999","No","No","No","Internal"]
[null,null,null,28657,30947,"0_Sat Jan 21 2023 05:34:55 GMT+0800","2023-01-11T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","General service air line, valves are leaking and same needs to be attended.","Deck - Pipe / Fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Leaking air valves replaced.","2023-05-26T23:59:09.999","","Completed","2023-05-08T23:59:09.999","No","No","No","Internal"]
[null,null,null,28658,99965,"0_Sat Jan 21 2023 05:36:08 GMT+0800","2023-01-11T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","Bunker manifold valves not holding same needs to be replaced.","Deck - Pipe / Fittings","MARPOL Related","Equipment Related","","","","","FO Bunker manifold valves (In total 4) replaced with new.  Line pressure tested at 4.4 bar. ","2023-08-31T23:59:09.999","","Completed","2023-08-30T23:59:09.999","No","No","No","Internal"]
[null,null,null,28659,63381,"55_Sat Jan 21 2023 05:57:16 GMT+0800","2023-01-11T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","Funnel damper valve cylinder and air valves found to be leaking","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Spares received and new air cylinder fitted, tested , working satisfactorily.","2023-07-29T23:59:09.999","SSUN230054","Completed","2023-07-19T23:59:09.999","No","No","No","Internal"]
[null,null,null,28660,59151,"55_Tue Jan 31 2023 23:30:48 GMT+0800","2023-01-20T23:59:09.999","Breakdown","Ship Staff","Ship Staff Insp.","Main Air Compressor No. 2 breakdown due to loose securing screw of gudgeon pin causing gudgeon pin to move causing damage.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Overhaul of compressor with used spares to keep it standby for emergency use. Vessel raised requisition for spares. There is no running issues with MAC at present, Since Main Air compressor No.2 has been running last 6 months-with vessel monitoring continuously with Vibration readings -defect closed.","2023-09-30T23:59:09.999","SSUN230033, SSUN230066 & SSUN230090","Completed","2023-09-28T23:59:09.999","No","No","No","Internal"]
[null,null,null,28858,95098,"55_Wed Feb 15 2023 08:57:00 GMT+0800","2023-01-29T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","Elevator inverter faulty and same needs to be replaced","Elect. Mach. & Equip.","","Equipment Related","","","","","Elevator inverter supplied, service engineer attended and same rectified","2023-02-20T23:59:09.999","ssun235007","Completed","2023-02-03T23:59:09.999","No","No","No","Internal"]
[null,null,null,28857,49227,"0_Wed Feb 15 2023 08:58:58 GMT+0800","2023-02-04T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","HFO Transfer pump coupling broken","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","","","","","transfer pump coupling renewed, pump tried out working satisfactory.","2023-06-12T23:59:09.999","SSUN230079","Completed","2023-06-07T23:59:09.999","No","No","No","Internal"]
[null,null,null,29370,41620,"55_Mon Mar 13 2023 11:19:22 GMT+0800","2023-02-14T23:59:09.999","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","SCBA compressor is used to charge both SCBA bottles and Lifeboat air bottles. \nSafety valve setting of 225 bar is for the safety of SCBA bottles. Does the vessel have separate safety valve when we are filling Lifeboat air bottle","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.43","High","","","Safety relief valve received","2023-07-14T23:59:09.999","","Completed","2023-07-03T23:59:09.999","No","No","No","Internal","This is a regulatory and a major safety issue and sooner or later will be pointed out during an external inspection. Please send us a separate mail and we will discuss this with the makers and advise the vessel to raise a new RO."]
[null,null,null,29372,69891,"55_Wed Mar 15 2023 16:36:07 GMT+0800","2023-02-14T23:59:09.999","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Starboard void space local gauge cable found damaged","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Spares received and changed the content guage. All found satisfactory. ","2024-02-01T23:59:09.999","SSUN230078","Completed","2024-01-25T23:59:09.999","No","No","No","Internal"]
[null,null,null,29374,69073,"55_Mon Mar 13 2023 11:12:48 GMT+0800","2023-02-14T23:59:09.999","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Crew members found drying up the clothes in the accommodation alley way","Accommodation","MLC Related","Behaviour Based","","","","","All clothes removed and crew members instructed not to dry clothes in alleyway. \nDedicated dry room and dryer to be used for the purpose. ","2023-03-08T23:59:09.999","","Completed","2023-02-22T23:59:09.999","No","No","No","Internal"]
[null,null,null,29375,84855,"55_Mon Mar 13 2023 11:25:17 GMT+0800","2023-02-14T23:59:09.999","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Receptacle for sound-powered telephone - cable insulation found damaged.","Miscellaneous","Communication","Equipment Related","","","","","Damaged Cable repaired. ","2023-03-24T23:59:09.999","","Completed","2023-02-23T23:59:09.999","No","No","No","Internal"]
[null,null,null,29376,86753,"55_Mon Mar 13 2023 11:32:29 GMT+0800","2023-02-14T23:59:09.999","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ER overhead crane hook secured with nylon slings. Change this to manila rope. ","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Human Error","","","","","Nylon Sling replaced with Manila Rope.","2023-03-24T23:59:09.999","","Completed","2023-02-23T23:59:09.999","No","No","No","Internal"]
[null,null,null,29377,82730,"55_Mon Mar 13 2023 11:36:30 GMT+0800","2023-02-14T23:59:09.999","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","5K250 valve in the ER found kept directly on the floor. To be kept on wooden plank","Miscellaneous","Eng. / Strg. Comp.","Human Error","","","","","Valve placed on wooden plank and secured. ","2023-03-24T23:59:09.999","","Completed","2023-02-25T23:59:09.999","No","No","No","Internal"]
[null,null,null,29378,23657,"55_Mon Mar 13 2023 11:39:17 GMT+0800","2023-02-14T23:59:09.999","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ME LOPx and FOPx feed temperature maintaining at 80-82 degC. \nTemperature to be maintained between 95-98 degC","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","","2023-03-24T23:59:09.999","","Completed","2023-02-27T23:59:09.999","No","No","No","Internal"]
[null,null,null,29379,17445,"55_Mon Mar 13 2023 11:44:41 GMT+0800","2023-02-14T23:59:09.999","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","24 alarms were in Off scanned condition during the visit. ","Miscellaneous","Eng. / Strg. Comp.","Behaviour Based","","","","","Same were removed from off scan during the visit. ","2023-03-24T23:59:09.999","","Completed","2023-02-14T23:59:09.999","No","No","No","Internal","Same were removed from off scan during the visit. "]
[null,null,null,29380,42136,"55_Mon Mar 13 2023 11:46:59 GMT+0800","2023-02-14T23:59:09.999","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Overwriting and corrections in the Engine  Log book were not counter signed by the Duty engineer","Documentation","Eng. / Strg. Comp.","Behaviour Based","","","","","All Overwriting and corrections in the Engine  Log book by Duty Engineer ","2023-03-24T23:59:09.999","","Completed","2023-02-23T23:59:09.999","No","No","No","Internal"]
[null,null,null,29381,79771,"55_Mon Mar 13 2023 11:49:33 GMT+0800","2023-02-14T23:59:09.999","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Wash basin in the ER found in very dirty condition","Miscellaneous","Eng. / Strg. Comp.","Behaviour Based","","","","","Wash Basin Cleaned.","2023-03-24T23:59:09.999","","Completed","2023-02-23T23:59:09.999","No","No","No","Internal"]
[null,null,null,29382,26724,"55_Mon Mar 13 2023 11:51:39 GMT+0800","2023-02-14T23:59:09.999","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Main Engine TC manometer to be filled with water","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","TC manometer filled with water","2023-03-24T23:59:09.999","","Completed","2023-02-25T23:59:09.999","No","No","No","Internal"]
[null,null,null,29383,28565,"55_Mon Mar 13 2023 11:53:50 GMT+0800","2023-02-14T23:59:09.999","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Few Quick closing valves in the ER found in very dirty condition. To be cleaned","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Quick closing valves cleaned.","2023-03-24T23:59:09.999","","Completed","2023-02-23T23:59:09.999","No","No","No","Internal"]
[null,null,null,29384,77014,"55_Mon Mar 13 2023 12:19:23 GMT+0800","2023-02-14T23:59:09.999","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","COP grease pots need to be filled up","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","","","","","COP grease pots filled up","2023-03-24T23:59:09.999","","Completed","2023-02-25T23:59:09.999","No","No","No","Internal"]
[null,null,null,29371,48420,"55_Tue Mar 14 2023 13:27:35 GMT+0800","2023-02-23T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","NO.1 AUX BOILER FD FAN BELLOW FOUND RUPTURED.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","AUX BOILER BELLOW REPLACED WITH SPARE NEW ONE","2023-07-18T23:59:09.999","","Completed","2023-07-18T23:59:09.999","No","No","No","Internal"]
[null,null,null,29373,27491,"55_Wed Mar 15 2023 23:19:43 GMT+0800","2023-02-26T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","HP DRUM GAUGE GLASS IS LEAKING.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Spare received, new gauge glass fitted.","2023-07-29T23:59:09.999","DSUN230029","Completed","2023-07-18T23:59:09.999","No","No","No","Internal"]
[null,null,null,29689,80798,"55_Sat Apr 01 2023 04:26:14 GMT+0800","2023-03-10T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","Water mist repeater panel on bridge PCB burnt","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","",""," PCB unit received after repairs last call Singapore and tested, found working satisfactorily..(Repaired PCB fitted in ECR Repeater panel)","2023-07-14T23:59:09.999","SSUN230039","Completed","2023-07-14T23:59:09.999","No","No","No","Internal"]
[null,null,null,29690,86114,"0_Sat Apr 01 2023 04:28:03 GMT+0800","2023-03-20T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","Various hydraulic fittings on staffa motor found to be rusted and same needs to be renewed.","Deck - Machinery,Deck - Mooring Machinery","Mooring","Equipment Related","9.14","Medium","","","Renewed leaky hydraulic fittings on mooring winch staffa motor.","2024-02-01T23:59:09.999","","Completed","2023-12-15T23:59:09.999","No","No","No","Internal","New fabricated spares have been supplied in Singapore and this job needs to be prioritized."]
[null,null,null,29968,68633,"55_Tue Apr 25 2023 22:01:14 GMT+0800","2023-03-25T23:59:09.999","Breakdown","Ship Staff","Ship Staff Insp.","RX-415, HC/O2 detector was found not giving “no pump suction” alarm. \nSimilarly, upon introducing calibration gas in normal mode there is no alarm activated when the O2 content falls. Also, the O2 reading does not go to zero on introducing 100% nitrogen. (Suspect internal leakage or faulty sensor)\n","Miscellaneous","Safety / LSA / FFA","Equipment Related","5.23","Very High","","","Received RX-415 along with rotation of Gas detectors. ","2023-06-25T23:59:09.999","SSUN235036","Completed","2023-07-03T23:59:09.999","No","No","No","Internal"]
[null,null,null,29974,61532,"55_Fri Apr 28 2023 05:06:26 GMT+0800","2023-04-02T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","NO.1 AUX BOILER IGNITION FLAME FAILURE TRIP AMPLIFIER IS NOT OPERATIONAL.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","TRIP AMPLIFIER CHANGED AND TRIED OUT WORKING SATISFACTORY.","2023-06-27T23:59:09.999","SSUN230085","Completed","2023-06-07T23:59:09.999","No","No","No","Internal"]
[null,null,null,29979,63213,"55_Mon May 01 2023 05:56:39 GMT+0800","2023-04-11T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","MAC 1  -Connecting rod bearing & Main bearing worn","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related","","","","","MAC I Complete overhaul -5000 hrs routine carried out, Bearings & Piston rings renewed.","2023-04-16T23:59:09.999","","Completed","2023-04-19T23:59:09.999","No","No","No","Internal"]
[null,null,null,29970,92219,"55_Tue Apr 25 2023 22:06:07 GMT+0800","2023-04-12T23:59:09.999","Observation","Ship Staff","Ship Staff Insp.","PORT LIFEBOAT ENTERANCE EMBARKATION RAILING FOUND TO HAVE CORRODED AND HAVING A HOLE   ","","Safety / LSA / FFA","Equipment Related","5.29","High","","","Lifeboat Access Door Railing, Top Railing removed found corroded \nNew railing fabricated. \nInstalled in location, Primer and final coat completed, covered with Tiger Strip Tape. ","2023-05-25T23:59:09.999","","Completed","2023-05-06T23:59:09.999","No","No","No","Internal"]
[null,null,null,29967,62460,"55_Tue Apr 25 2023 21:59:20 GMT+0800","2023-04-13T23:59:09.999","Observation","Ship Staff","Ship Staff Insp.","Hoisting wire on port side ladder to sunken deck from upper deck, has only two turns on the drum","Deck - Machinery","Safety / LSA / FFA","Equipment Related","5.47","Medium","","","Port Side ISPS Ladder, heaved up during test and checks for transiting Malacca and Singapore straights found in working order.  \n ","2023-06-25T23:59:09.999","SSUN230121","Completed","2023-05-26T23:59:09.999","No","No","No","Internal"]
[null,null,null,29966,94549,"55_Tue Apr 25 2023 21:57:29 GMT+0800","2023-04-15T23:59:09.999","Observation","Ship Staff","Ship Staff Insp.","STBD WINDLASS, MOORING DRUMS AND FITTINGS JERKING DURING LOWERING/SLACKNING","Deck - Mooring Machinery","Mooring","Equipment Related","","","","","","2023-09-15T23:59:09.999","","Completed","2023-06-14T23:59:09.999","No","No","No","Internal"]
[null,null,null,30243,91461,"55_Tue May 16 2023 02:30:52 GMT+0800","2023-04-16T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","Starboard Bridge Wing ME Control unit BWU09-Lever (Telegraph), pot meter faulty.","E/R - Main Engine","Navigation","Equipment Related","10.32","Very High","","","Starboard Bridge Wing ME Control unit LTU was replaced with spare one by Service engineer. Tested and found satisfactory. ","2023-11-30T23:59:09.999","","Completed","2023-11-24T23:59:09.999","No","No","No","Internal","Service attendance will be planned from Kongsberg from makers "]
[null,null,null,29971,10140,"55_Tue Apr 25 2023 22:07:24 GMT+0800","2023-04-17T23:59:09.999","Observation","Ship Staff","Ship Staff Insp.","TORCH FOR FIRE MAN OUTFITS, FOUND TO BE OF LESS INTENSITY. ","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.43","High","","","Replacement received and placed at designated locations. ","2023-06-25T23:59:09.999","SSUN230086","Completed","2023-06-07T23:59:09.999","No","No","No","Internal"]
[null,null,null,29972,83186,"55_Tue Apr 25 2023 22:08:12 GMT+0800","2023-04-17T23:59:09.999","Observation","Ship Staff","Ship Staff Insp.","GLOVES FOR FIREMAN OUTFITS (2 SETS) ARE SMALL SIZE, DOES NOT FIT TO MANY CREW MEMBERS.","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.43","High","","","Spares received and placed at designated locations. ","2023-06-25T23:59:09.999","SSUN230086","Completed","2023-06-07T23:59:09.999","No","No","No","Internal"]
[null,null,null,29973,17971,"55_Thu Apr 27 2023 18:03:34 GMT+0800","2023-04-17T23:59:09.999","Breakdown","Ship Staff","Ship Staff Insp.","Neil Robertson Stretcher in Pumproom, found with strap broken. ","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.20","Medium","","","Broken Strap Stitched, and stretcher put back in location. ","2023-05-27T23:59:09.999","","Completed","2023-04-28T23:59:09.999","No","No","No","Internal"]
[null,null,null,29978,77101,"55_Tue Apr 25 2023 22:03:25 GMT+0800","2023-04-17T23:59:09.999","Observation","Ship Staff","Ship Staff Insp.","BREATHER VALVE FOR INERT GAS LINE FOUND TO BE PASSING AT PRESSURE GREATER THAN 400 MMWG","Cargo Mach.","Safety / LSA / FFA","Equipment Related","8.41","Medium","","","breather valve removed from location, found to have pittings, same have been attended and boxed back. Once IG is Topped Up will monitor again for any signs of leaks. Presently no leak noticed till 400 mmwg. ","2023-06-25T23:59:09.999","","Completed","2023-04-23T23:59:09.999","No","No","No","Internal"]
[null,null,null,29976,83047,"55_Mon May 01 2023 07:14:23 GMT+0800","2023-04-18T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","Unable to connect the Intrinsically Safe Camera provided for use on Deck to any of the Computers, including Master’s Computer.\nUpon connecting to any device “USB Device Not Recognized” Warning is flashed.\nDetails of the phone are \nModel Number: Impact X\nDevice Name: Impact X-PXIMEX14006225\nAndroid Version 5.1.1\nBluetooth transferring was tested, did not happen.\n","Miscellaneous","Safety / LSA / FFA","Equipment Related","5.6","Low","","","It is not getting connected with the supplied USB cable but it got connected by the crew’s USB cable. Same was tested on Ship’s Computer, and the phone got connected using crew’s USB cable. The supplied USB cable is only charging the device and is not supporting file transfer.  Requisition has been raised for same. \n","2023-07-18T23:59:09.999","SSUN230083","Completed","2023-05-14T23:59:09.999","No","No","No","Internal"]
[null,null,null,29969,20036,"55_Tue Apr 25 2023 22:02:29 GMT+0800","2023-04-19T23:59:09.999","Breakdown","Ship Staff","Ship Staff Insp.","JOINING ANGLE BETWEEN RAILINGS (NEAR OP 285) IN PUMPROOM ON STAIR CASE LEADING TO TRO UNIT PLATFORM FOUND BROKEN FROM ONE END.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","","","","","Bracket and Bolt Arrangement made and railings secured, \nPrimer and Final Coat Applied. ","2023-06-25T23:59:09.999","","Completed","2023-04-29T23:59:09.999","No","No","No","Internal"]
[null,null,null,29977,80031,"55_Mon May 01 2023 07:26:36 GMT+0800","2023-04-24T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","AFT ETA,  Towing Pennant Drum Found Seized and Unmovable during Routine Inspection and Drills","LSA / FFA","Safety / LSA / FFA","Equipment Related","9.28","Medium","","","Break had got seized due to rusting, same was dismantled and cleared of all corrosion. \nTested for operation, working satisfactory. ","2023-06-02T23:59:09.999","","Completed","2023-04-28T23:59:09.999","No","No","No","Internal"]
[null,null,null,30241,91988,"55_Thu May 11 2023 23:07:36 GMT+0800","2023-04-28T23:59:09.999","Defect","Ship Staff","Ship Staff Insp."," AUS pumps casing temperature gauges are not working.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.80","Medium","","","New spares received, installed and made operational.","2023-10-15T23:59:09.999","SSUN230102","Completed","2023-10-09T23:59:09.999","No","No","No","Internal"]
[null,null,null,30244,99906,"55_Thu May 11 2023 23:11:23 GMT+0800","2023-04-28T23:59:09.999","Observation","Ship Staff","Ship Staff Insp.","Steering Gear Walkway Gratings are not secured","Miscellaneous","Eng. / Strg. Comp.","Inappropriate Procedure","10.43","Medium","","","Steering gear room walkway gratings secured.","2023-05-27T23:59:09.999","","Completed","2023-05-15T23:59:09.999","No","No","No","Internal"]
[null,null,null,30242,95702,"55_Fri May 12 2023 19:07:48 GMT+0800","2023-04-30T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","IG AND IGG SCRUBBER OVBD VALVES REMOTE OPERATION INDICATION JUNCTION BOX ES AT SUNKEN DECK ARE COMPLETELY WASTED.","Elect. Mach. & Equip.","General Appearance","Equipment Related","10.37","Medium","","","All junction boxes were covered by a separate metal cover to cover the complete valve along with the junction boxes, All cable connections were properly secured.","2023-07-29T23:59:09.999","","Completed","2023-07-20T23:59:09.999","No","No","No","Internal"]
[null,null,null,30345,96871,"55_Fri Jun 02 2023 15:34:00 GMT+0800","2023-05-13T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","Main engine no.1 unit exhaust valve stroke sensor is faulty.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","storke sensor replaced with new one after stopping main engine, now working satisfactory.","2023-05-28T23:59:09.999","","Completed","2023-05-23T23:59:09.999","No","No","No","Internal"]
[null,null,null,30342,35263,"55_Fri Jun 02 2023 08:45:58 GMT+0800","2023-05-29T23:59:09.999","Observation","Ship Staff","Ship Staff Insp.","BWTS TRO Detection Cabinets AIT-151 & AIT-251, should show Green Light for Pressure, Timer & By-Pass at all times. The Light for Pressure and By-Pass are turning to Red after some interval. Suspect leak of Positive Pressure or insufficient positive pressure. ","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.13","Medium","","","Another Thin Gasket has been placed underneath the Original Gasket inside the Cabinet Door, to increase the area of contact. \nPresently all 3 lights are showing green. ","2023-06-27T23:59:09.999","","Completed","2023-06-07T23:59:09.999","No","No","No","Internal"]
[null,null,null,30344,33052,"55_Fri Jun 02 2023 20:47:03 GMT+0800","2023-05-30T23:59:09.999","Observation","Ship Staff","Ship Staff Insp.","Minor seepage noticed in VRCS Return Line under U Clamp, in vicinity of Foam Monitor # 7","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.11","Medium","","","Section cropped and replaced. \nPut back in location and system tested, found in order. ","2023-06-27T23:59:09.999","","Completed","2023-05-31T23:59:09.999","No","No","No","Internal"]
[null,null,null,30499,47217,"55_Tue Jun 13 2023 17:29:04 GMT+0800","2023-05-31T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","AFT HYDRAULIC MACHINERY ALARMS ARE NOT CONNECTED TO AMS PANEL.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","FAULT RECTIFIED AND ALARM TESTED, WORKING SATISFACTORY","2023-07-17T23:59:09.999","","Completed","2023-08-08T23:59:09.999","No","No","No","Internal"]
[null,null,null,30501,75636,"55_Mon Jun 12 2023 15:58:04 GMT+0800","2023-05-31T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","OILY WATER SEPERATOR FLOW SWITCH OPERATION IS ERRATIC.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Spare received and replaced with new one. ","2024-02-01T23:59:09.999","SSUN230124","Completed","2024-01-25T23:59:09.999","No","No","No","Internal"]
[null,null,null,30500,46875,"55_Thu Jun 15 2023 15:29:29 GMT+0800","2023-06-03T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","No.1 FWG Ejector pump discharge valve to the EGB washing line is having a pinhole.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.31","Very High","","","Vessel changed the FWG ejector pump No. 1 discharge valve to WHRS wash water line with new spare. Valve tested while water washing WHRS.","2023-10-30T23:59:09.999","SSUN230185","Completed","2023-10-12T23:59:09.999","No","No","No","Internal"]
[null,null,null,30502,60315,"55_Thu Jun 15 2023 15:33:07 GMT+0800","2023-06-04T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","EGB drain valve is not holding smoke is leaking to soot tank","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.31","Very High","","","EGB drain valve to soot tank replaced with new, which was received during vessels last call at Singapore.","2023-08-10T23:59:09.999","","Completed","2023-08-04T23:59:09.999","No","No","No","Internal"]
[null,null,null,30948,23198,"55_Sat Jul 01 2023 09:24:55 GMT+0800","2023-06-24T23:59:09.999","Observation","Owner / Marine / Tech. Suptd.","Ship Staff Insp.","AUX ENGINE AIR SCAVENGE MANIFOLD DRAIN LINES TO BE SEPRATED FROM DRAIN BOX AND FITTED INDIVIDUALLY WITH  3MM ORIFICE.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","ALL DRAIN LINES SEPARATED , BALL VALVE  INSTALLED KEPT OPEN -REGULATED TO MONITOR DRAINS ARE CLEAR.","2023-07-30T23:59:09.999","","Completed","2023-07-12T23:59:09.999","No","No","No","Internal"]
[null,null,null,30943,75923,"55_Sat Jul 15 2023 23:14:36 GMT+0800","2023-07-03T23:59:09.999","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Fwd and after hydraulic motor for deck power pack, does not have any inspection hole for inspection of coupling. \t\t","Deck - Machinery","Mooring","Equipment Related","","","","","Hole Made as instructed.","2023-08-10T23:59:09.999","","Completed","2023-08-02T23:59:09.999","No","No","No","Internal"]
[null,null,null,30944,58604,"55_Sat Jul 15 2023 23:16:31 GMT+0800","2023-07-03T23:59:09.999","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","On main deck Walkway stanchion wire in corroded condition\t\t","Miscellaneous","Safety / LSA / FFA","Equipment Related","","","","","Wires de rusted and greased. ","2023-08-30T23:59:09.999","","Completed","2023-07-24T23:59:09.999","No","No","No","Internal"]
[null,null,null,30945,96170,"55_Sun Jul 16 2023 03:27:38 GMT+0800","2023-07-03T23:59:09.999","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Engine room Blower casing to de-rust and paint","Miscellaneous","General Appearance","Equipment Related","","","","","Blower casing  de-rusted and painted","2023-10-03T23:59:09.999","","Completed","2023-09-18T23:59:09.999","No","No","No","Internal","Maintenance to be prioritized "]
[null,null,null,30946,62384,"55_Sun Jul 16 2023 03:30:43 GMT+0800","2023-07-03T23:59:09.999","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Engine Casing Funnel spot rust to touch up","Deck - Pipe / Fittings","General Appearance","Equipment Related","","","","","Funnel Casing Forward, Port and Stbd side bulkhead spot de-rusted, primer and final coat completed.","2023-08-14T23:59:09.999","","Completed","2023-08-08T23:59:09.999","No","No","No","Internal"]
[null,null,null,30947,23839,"55_Sat Jul 15 2023 23:18:00 GMT+0800","2023-07-03T23:59:09.999","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Water collected in the stripping pump save all. TO find the source of leak and rectify","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","Water was drained during the Warming Up procedure of the stripper pump as vessel had used stripper pump for de slopping at Singapore on 04 Aug 23. \nAll water from drip tray has been removed and cleaned.  ","2023-07-21T23:59:09.999","","Completed","2023-07-07T23:59:09.999","No","No","No","Internal"]
[null,null,null,32850,56552,"55_Fri Oct 20 2023 14:50:03 GMT+0800","2023-07-14T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","VRCS system main line pressure relief valve is leaking, causing frequent loading/unloading of unloader for running pump and frequent cut in/cut off of stand by pump.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.30","High","","","Replaced the relief valve and system tried out. System is operational and tried out during one loading and discharging operation.","2024-03-01T23:59:09.999","DSUN230153","Completed","2024-02-23T23:59:09.999","No","No","No","Internal"]
[null,null,null,31687,38450,"55_Tue Aug 22 2023 01:51:57 GMT+0800","2023-08-01T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","Gear Oil Dripping Leak noticed on Port Side Windlass, from underneath the shaft in between the Windlass and the Inboard mooring rope drum.   ","Deck - Machinery","Mooring","Equipment Related","9.20","Medium","","","Breather valve found seized same pressurising gear case, same eased up. Oil level maintained in the sight glass. Operation checked and no leaks observed.","2024-01-01T23:59:09.999","","Completed","2023-10-28T23:59:09.999","No","No","No","Internal"]
[null,null,null,31691,56801,"55_Tue Aug 22 2023 01:42:52 GMT+0800","2023-08-08T23:59:09.999","Breakdown","Ship Staff","Ship Staff Insp.","Aft Mooring Winch Motor - Return Line For Hydraulic Oil, Soft Patch Formation and Leaking. \n","Deck - Pipe / Fittings","Mooring","Equipment Related","11.4","Very High","","","Permanent repaired carried out, by crop and renew the stub piece.Hydraulic return line tested after repair, found in order.\n","2023-11-30T23:59:09.999","","Completed","2023-11-19T23:59:09.999","No","No","No","Internal"]
[null,null,null,31688,95600,"55_Sat Aug 26 2023 02:49:59 GMT+0800","2023-08-13T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","BWTS Neutralization pump discharge line going to pump room has several leaks in engine room. Leaks are due to material failure of the discharge tubing.","E/R - Pipes/ valves & fittings","Cargo / Ballast Systems","Equipment Related","","","","","All lines renewed with new material supplied. Line pressure tested after repair and found in good order.","2023-10-30T23:59:09.999","SSUN230164 (Received onboard)","Completed","2023-10-27T23:59:09.999","No","No","No","Internal"]
[null,null,null,31689,22721,"55_Wed Aug 30 2023 08:11:02 GMT+0800","2023-08-26T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","Water Ballast Tank Fixed Gas Detection System Giving Internal Leakage Alarm Repeatedly ","Deck - Machinery","Cargo / Ballast Systems","Equipment Related","","","","","Both sampling pump diaghram renewed and system made operational without any alarm.","2023-10-30T23:59:09.999","","Completed","2023-09-08T23:59:09.999","No","No","No","Internal"]
[null,null,null,31900,85428,"55_Fri Sep 15 2023 09:51:22 GMT+0800","2023-09-01T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","Main engine Start air pipe for No.6 Unit is holed","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.1","Medium","","","Start Air pipe was removed and repairs carried out by welding.  Presently its working fine.","2023-10-10T23:59:09.999","SSUN230177","Completed",null,"No","No","No","Internal"]
[null,null,null,31903,30930,"55_Thu Sep 14 2023 17:43:54 GMT+0800","2023-09-03T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","ME No.1 Unit Cylinder cover crack confirmed from leak through Star air pipe pocket-finding its way to Start air manifold","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.10","High","","","Replaced cylinder cover for Unit No.1 ","2023-09-05T23:59:09.999","","Completed","2023-09-04T23:59:09.999","No","No","No","Internal"]
[null,null,null,31902,57113,"55_Fri Sep 15 2023 09:59:17 GMT+0800","2023-09-04T23:59:09.999","Defect,Non Conformity","Ship Staff","Ship Staff Insp.","ME No.1 Unit Liner Jacket l(Lower) has a crack.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","ME unit Cylinder liner removed and new Lower Liner water jacket installed. Job carried out by Shore Workshop at Singapore","2023-09-12T23:59:09.999","","Completed","2023-09-12T23:59:09.999","No","No","No","Internal"]
[null,null,null,31893,94141,"55_Thu Sep 14 2023 11:39:02 GMT+0800","2023-09-11T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","VECS Oxygen Sensor at Manifold not giving correct reading of Oxygen Level ","Inert Gas","Safety / LSA / FFA","Equipment Related","8.17","Low","","","All sampling lines, unions, and flowmeter cleared as same were blocked with carbon deposits. Damaged sampling lines renewed. Sensor calibrated and system observed for 3 days. System found to be operating normal.\n","2023-10-31T23:59:09.999","","Completed","2023-10-30T23:59:09.999","No","No","No","Internal"]
[null,null,null,31901,94074,"55_Fri Sep 29 2023 00:08:23 GMT+0800","2023-09-12T23:59:09.999","Breakdown","Ship Staff","Ship Staff Insp.","Engine room crane High Hoist motor not working-Motor shaft spline sheared off","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","New hoisting motor along with brake assembly installed. Engine room crane load tested and put in service.","2023-10-05T23:59:09.999","SSUN 230190 & SSUN230040","Completed","2023-10-05T23:59:09.999","No","No","No","Internal"]
[null,null,null,31896,68681,"55_Fri Sep 29 2023 00:32:17 GMT+0800","2023-09-24T23:59:09.999","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Overboard pipe of EGCS-GRP near AE's -pipe flange to have splash-Guards around -to avoid water splash on AE's .","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.23","Medium","","","Fabrication and installation of guard cover for GRP Pipe flanges using GI Sheets is complete. All flanges of EGCS overboard pipe near auxiliary engines have anti-splash protection cover.","2023-11-30T23:59:09.999","","Completed","2023-10-28T23:59:09.999","No","No","No","Internal"]
[null,null,null,31899,64187,"55_Fri Sep 29 2023 00:50:10 GMT+0800","2023-09-24T23:59:09.999","Defect,Observation","Ship Staff","Ship Staff Insp.","The drains for Funnel deck save all drain line are  choked and the water does not drain from the save all-as a result the water splashes on to the electrical Lamp fitting.(Near Port side ER Blower)","Deck - Pipe / Fittings","General Appearance","Equipment Related","","","","","Drains cleared.","2023-10-30T23:59:09.999","","Completed","2023-10-27T23:59:09.999","No","No","No","Internal"]
[null,null,null,31897,94311,"55_Fri Sep 29 2023 00:36:21 GMT+0800","2023-09-27T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","EGCS Effluent flow sensor defective -PCB Burnt","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.11","Medium","","","New EGCS Effluent flow sensor received in Singapore transit and was changed. Now, its operational. ","2024-02-01T23:59:09.999","SSUN230193","Completed","2024-01-06T23:59:09.999","No","No","No","Internal"]
[null,null,null,32858,99712,"55_Tue Oct 31 2023 10:04:10 GMT+0800","2023-10-18T23:59:09.999","Breakdown","Ship Staff","Ship Staff Insp.","NO. 1 Air condition compressor controller unit found with no power / display. Main PCB was defective.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.30","High","","","AC controller unit (Type ACS 2) replaced with new spare. Unit programmed and put in service.","2023-11-01T23:59:09.999","","Completed","2023-10-25T23:59:09.999","No","No","No","Internal"]
[null,null,null,32851,66198,"55_Tue Oct 31 2023 09:51:57 GMT+0800","2023-10-22T23:59:09.999","Breakdown","Ship Staff","Ship Staff Insp.","HFO purifier No. 2 pneumatically operated 3-way valve malfunctioning. Operation of 3-way valve is erratic due to improper sealing of air piston & cylinder. ","E/R - Purifier","Eng. / Strg. Comp.","Equipment Related","10.3","Medium","","","Replaced the 3 way valve with new spare received. System tried out. All found satisfactory. ","2024-02-07T23:59:09.999","SSUN230203","Completed","2024-02-03T23:59:09.999","No","No","No","Internal","Spares will be arranged at Singapore in Jan 2024."]
[null,null,null,32857,91244,"55_Mon Oct 30 2023 20:28:17 GMT+0800","2023-10-22T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","STBD crane block sheeve is in ceased condition.","Deck - Machinery","Safety / LSA / FFA","Equipment Related","8.50","Medium","","","STBD crane block sheeves removed from crane block. De rusting, painting freeing up carried out on the same and put back in position. ","2023-11-01T23:59:09.999","","Completed","2023-10-27T23:59:09.999","No","No","No","Internal"]
[null,null,null,32856,62737,"55_Mon Oct 30 2023 20:17:44 GMT+0800","2023-10-23T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","Both port and stbd gangway sheeves are in rusted condition.","Deck - Pipe / Fittings","Safety / LSA / FFA","Equipment Related","5.47","Medium","","","Port and stbd accommodation ladder sheeves removed. Freeing up, de rusting and painting, greasing carried out on same and put back in position.  ","2023-10-31T23:59:09.999","","Completed","2023-10-29T23:59:09.999","No","No","No","Internal"]
[null,null,null,32861,45728,"55_Tue Oct 31 2023 16:45:48 GMT+0800","2023-10-29T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","Foam monitor no.7 valve is in ceased condition.","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.38","High","","","Overhauling / freeing up of no7 foam isolation valve carried out, Pressure testing of same done, found in order.\n","2023-11-03T23:59:09.999","","Completed","2023-11-02T23:59:09.999","No","No","No","Internal"]
[null,null,null,32859,80019,"55_Tue Oct 31 2023 10:12:27 GMT+0800","2023-10-31T23:59:09.999","Breakdown","Ship Staff","Ship Staff Insp.","HFO purifier No. 2 motor found making abnormal noise. Motor insulation recorded as 0.5 Mega-ohms.   ","E/R - Purifier","Eng. / Strg. Comp.","Equipment Related","10.3","Medium","","","Vessel installed one spare motor of same model with 22 Kw rating (Original motor with 26 Kw rating),  New contactor received and installed for starting panel. Purifier tried out and found working satisfactory.","2023-12-01T23:59:09.999","SSUN230208 - El. Motor\nSSUN230211 - Magnetic contactor for starter panel","Completed","2023-11-22T23:59:09.999","No","No","No","Internal"]
[null,null,null,32852,47931,"55_Wed Nov 08 2023 10:24:44 GMT+0800","2023-11-09T23:59:09.999","Other","Ship Staff","Ship Staff Insp.","Vessel is fitted with Fixed CO2 fire extinguishing system for machinery space, pump room & emergency generator room, manufactured by NK Co. LTD. The manufacturing date for the system is 01-NOV-2011. Vessel received Marine safety advisory notice No. 14 of 2023, which states, \"change of material of bursting disc on carbon dioxide cylinder valves from copper to nickel\". The cylinder valve will have to be changed to renew bursting disc. ","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","Cylinder valves for individual carbon dioxide cylinders will have to be changed to renew bursting disc. The job has been shifted to REFMAN.","2027-01-02T23:59:09.999","","Completed","2023-12-06T23:59:09.999","No","No","No","Internal"]
[null,null,null,32860,69330,"55_Thu Nov 30 2023 20:28:28 GMT+0800","2023-11-29T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","No.3 STBD side window wiper was not operational. ","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","On investigation, found belt broken. Same replaced with spare new belt. Tested and working satisfactory. ","2023-12-01T23:59:09.999","","Completed","2023-12-01T23:59:09.999","No","No","No","Internal"]
[null,null,null,33323,77696,"55_Fri Dec 15 2023 16:01:01 GMT+0800","2023-12-08T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","Running hour meter for Service air compressor was in-operational. ","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related","10.3","Medium","","","Running hour meter for Service air compressor was replaced with spare new one. ","2023-12-14T23:59:09.999","","Completed","2023-12-09T23:59:09.999","No","No","No","Internal"]
[null,null,null,33320,14858,"55_Fri Dec 15 2023 15:34:45 GMT+0800","2023-12-09T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","Port side Hose handling crane heaving limit was rusted but operational. ","Deck - Machinery","Cargo / Ballast Systems","Equipment Related","9.20","Medium","","","The limit switch was replaced with spare new one and the rusted one cleaned and  lubricated.  ","2023-12-09T23:59:09.999","","Completed","2023-12-09T23:59:09.999","No","No","No","Internal"]
[null,null,null,33322,21713,"0_Fri Dec 15 2023 15:48:18 GMT+0800","2023-12-12T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","While carrying out the calibration of the inlet water analyser of the EGCS System, found the drain pipe of the scupper obstructing the placement of the portable display unit of EGCS. ","E/R - Aux. Mach.","Eng. / Strg. Comp.","External Factors","10.30","High","","","The drain pipe above the inlet analyser was removed and modified and fitted back. ","2023-12-17T23:59:09.999","","Completed","2023-12-16T23:59:09.999","No","No","No","Internal"]
[null,null,null,33321,48224,"0_Fri Dec 15 2023 15:38:18 GMT+0800","2023-12-13T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","When trying out AE LO purifier, found lube oil leaking from end flange of the heater. ","E/R - Purifier","Eng. / Strg. Comp.","Equipment Related","10.30","High","","","Purifier was stopped. Heater drained and the element was removed from place. Gaskets renewed and system tried out and found no leaks. ","2023-12-15T23:59:09.999","","Completed","2023-12-14T23:59:09.999","No","No","No","Internal"]
[null,null,null,33324,13889,"55_Fri Dec 15 2023 15:58:30 GMT+0800","2023-12-16T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","During routine inspection, Steering gear room phone cord was found to be brittle. ","Elect. Mach. & Equip.","Eng. / Strg. Comp.","External Factors","11.10","Medium","","","Phone cord was replaced with spare new one. ","2023-12-16T23:59:09.999","","Completed","2023-12-16T23:59:09.999","No","No","No","Internal"]
[null,null,null,25640,81664,"0_Wed Jun 15 2022 02:48:19 GMT+0800","2023-12-31T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","WHRS soot blow not possible from ECR panel.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Spares received and installed on by service engineer. System could not be tried out in presence of service engineer with ME stopped.\nSystem tried out at sea but found no response from ECR control as well as from local control panel. Communication with office and maker in progress. Presently, soot blow of EGB is carried out from local control panel. ","2024-08-01T23:59:09.999","SSUN230029","Completed","2024-06-02T23:59:09.999","No","No","No","Internal","office correspondence in progress"]
[null,null,null,38465,22356,"55_Mon Jan 06 2025 20:59:37 GMT+0800","2024-01-02T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","NO.2 DG Unit No.5 Main Bearing temperature reading found to be erractic and giving alarm\n","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Stopped the DG and found the temperature sensor to be defective. Replaced with spare one onboard and DG started. All found satisfactory. \n","2024-01-06T23:59:09.999","","Completed","2024-01-06T23:59:09.999","No","No","No","Internal"]
[null,null,null,34477,16437,"55_Mon Jan 08 2024 16:08:41 GMT+0800","2024-01-02T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","NO.2 DG Unit No.5 Main Bearing temperature reading found to be erractic and giving alarm","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.30","High","","","Stopped the DG and found the temperature sensor to be defective. Replaced with spare one onboard and DG started. All found satisfactory. ","2024-01-06T23:59:09.999","","Completed","2024-01-06T23:59:09.999","No","No","No","Internal"]
[null,null,null,36409,17230,"55_Sat Jun 01 2024 17:25:47 GMT+0800","2024-01-11T23:59:09.999","Observation","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","Item 5.6.1.1 paragraph(3) double hull construction in Form B of IOPP Certificate was not ticked as applicable for this tanker.","Hull & Tanks","Cert. & Docu.","Inappropriate Procedure","8.4","Medium","","","Immediately contacted LR Class and rectified.",null,"","Completed","2024-01-18T23:59:09.999","No","No","No","External"]
[null,null,null,36410,88161,"0_Sat Jun 01 2024 17:35:36 GMT+0800","2024-01-11T23:59:09.999","Observation","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","Fire hose with one fire hydrant nearby starboard side main engine bottom platform was 20 metre in length.","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.41","Very High","","","Immediately Hose renewed with correct length.",null,"","Completed","2024-01-11T23:59:09.999","No","No","No","External"]
[null,null,null,36413,52083,"0_Sat Jun 01 2024 17:30:49 GMT+0800","2024-01-11T23:59:09.999","Observation","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","No lagging provided for both  aux. boilers inspection holes and sighting port. Risk of scalding was not taken into consideration.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Immediately Rectified.",null,"","Completed","2024-01-11T23:59:09.999","No","No","No","External"]
[null,null,null,34472,84147,"55_Thu Jan 11 2024 16:17:18 GMT+0800","2024-01-12T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","NO.1 IG BLOWER MOTOR FAN BROKEN ","","Cargo / Ballast Systems","Equipment Related","","","","","new fan received against requisition and fitted.","2024-05-01T23:59:09.999","SSUN240031","Completed",null,"No","No","No","Internal"]
[null,null,null,30343,32504,"55_Fri Jun 02 2023 10:15:42 GMT+0800","2024-01-20T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","The EGCS Scrubber Absorber Bottom plate has a minor crack at the welding seam.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Cold Repair was carried out inside the Scrubber Absorber and additional Support was fitted to avoid Flexing of bottom plate, kept under close monitioring. Defect kept open till further instructions from Office /maker. Leak is under observation. ","2024-08-01T23:59:09.999","","Completed","2024-06-05T23:59:09.999","No","No","No","Internal"]
[null,null,null,34480,65187,"55_Fri Feb 02 2024 13:08:38 GMT+0800","2024-01-25T23:59:09.999","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Numerous breather valves on mooring winches have been found painted and ring missing to pull out the breather valve.","Deck - Mooring Machinery","Mooring","Equipment Related","9.14","Medium","","","Breather valve on all mooring winches free from paint and in working order. RIngs fitted as applicable ","2024-02-25T23:59:09.999","","Completed","2024-03-01T23:59:09.999","No","No","No","Internal"]
[null,null,null,39962,85912,"0_Thu Mar 20 2025 03:57:44 GMT+0800","2024-01-27T23:59:09.999","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Thermometer for No 1 unit and ME Jacket Fresh water not working","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Thermometer for NO1 unit and ME Jacket fresh water renewed ","2024-02-11T23:59:09.999","","Completed","2024-02-06T23:59:09.999","No","No","No","Internal"]
[null,null,null,39963,41872,"0_Thu Mar 20 2025 03:59:36 GMT+0800","2024-01-27T23:59:09.999","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","The winch brake locking nuts were not in compliance with MEG4","Deck - Mooring Machinery","Mooring","Equipment Related","","","","","Markings carried out in line with MEG4. Separate pointers fixed on mooring winches.","2024-02-11T23:59:09.999","","Completed","2024-02-02T23:59:09.999","No","No","No","Internal"]
[null,null,null,39964,87261,"0_Thu Mar 20 2025 04:02:03 GMT+0800","2024-01-27T23:59:09.999","Non Conformity","Owner / Marine / Tech. Suptd.","Suptd. Insp.","As per SOLAS 3 - 19.4.2: Records of Training not sighted\na. Hypothermia + FA treatment\nb. Use of ships LSA in severe weather","Documentation","Cert. & Docu.","Human Error","","","","","Training for the same carried out as per SOLAS Ch3.","2024-02-03T23:59:09.999","","Completed","2024-01-29T23:59:09.999","No","No","No","Internal"]
[null,null,null,39966,36064,"55_Thu Mar 20 2025 03:51:08 GMT+0800","2024-01-27T23:59:09.999","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Port and stbd anchor hawse pipe covers found one plate distorted and anchor bolts adrift","Deck - Pipe / Fittings","ISPS Related","Equipment Related","","","","","Distorted plate renewed and anchor bolts secured","2024-02-11T23:59:09.999","","Completed","2024-02-03T23:59:09.999","No","No","No","Internal"]
[null,null,null,39967,83156,"0_Thu Mar 20 2025 03:52:43 GMT+0800","2024-01-27T23:59:09.999","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Crew CBA for Indian officers for 2024 not available","Documentation","Cert. & Docu.","Human Error","","","","","Crew CBA for Indian Officers placed ","2024-02-06T23:59:09.999","","Completed","2024-01-30T23:59:09.999","No","No","No","Internal"]
[null,null,null,39968,66807,"0_Thu Mar 20 2025 03:54:31 GMT+0800","2024-01-27T23:59:09.999","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Wheelshouse Aircon Not working and RO pending - Must attend to prior summer sets in northern hemisphere","Accommodation","Navigation","Equipment Related","","","","","New Aircon fixed on bridge","2024-03-26T23:59:09.999","","Completed","2024-02-25T23:59:09.999","No","No","No","Internal"]
[null,null,null,39969,55665,"0_Thu Mar 20 2025 03:56:15 GMT+0800","2024-01-27T23:59:09.999","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Coir(Secondary) fenders were not standby on deck prior bunkering operation","Deck - Mooring Machinery","Mooring","Inappropriate Procedure","","","","","All crew briefed about the same and were informed to keep coir fenders standby fwd and aft station during the bunkering operations","2024-02-11T23:59:09.999","","Completed","2024-01-29T23:59:09.999","No","No","No","Internal"]
[null,null,null,34478,68226,"55_Fri Feb 02 2024 11:22:25 GMT+0800","2024-01-28T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","Pressure gauges of Aft Hydraulic pump No.1 and No.2 were defective. ","Deck - Mooring Machinery","Eng. / Strg. Comp.","Equipment Related","9.20","Medium","","","Replaced with pressure gauges with spare new one. ","2024-02-02T23:59:09.999","","Completed","2024-01-29T23:59:09.999","No","No","No","Internal"]
[null,null,null,31898,97379,"55_Fri Sep 29 2023 00:44:12 GMT+0800","2024-02-09T23:59:09.999","Observation","Ship Staff","Ship Staff Insp.","Various Air trunkings in Engine room-IG Blower platform, BWTS Room, Near Aux boiler 2-Staircase needs to be repaired-Including flap for IG Blower Air trunk.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.18","High","","","Vessel  attempted IG b lower Platform air trunking. It was wasted in middle. Same patched up with cold repair and its working fine.  Vessel will attempt for Boiler Area and BWTS platform at the earliest oppurtunity. ","2024-08-31T23:59:09.999","","Completed","2024-06-06T23:59:09.999","No","No","No","Internal"]
[null,null,null,34483,55697,"55_Thu Feb 15 2024 14:43:49 GMT+0800","2024-02-10T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","No.1 HFO purifier supply pump magnectic coupling cover housing damaged. ","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","No.1 HFO purifier supply pump opened up and on inspection found the bearing damaged. Same replaced with new spare one. Pump rotor magnectic coupling replaced as it was damaged too. All gaskets and O rings changed. Pump tried out. All found satisfactory. ","2024-02-11T23:59:09.999","","Completed","2024-02-11T23:59:09.999","No","No","No","Internal"]
[null,null,null,34479,65451,"55_Thu Feb 15 2024 14:40:24 GMT+0800","2024-02-13T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","No.1 Economiser Feed Pump observed to be having vibration from the pump end. ","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","The Pump was opened up for inspection. On inspection, found the shaft bearing close to the motor coupling worn out and Intermediate sleeve missing. Same replaced with spare one onboard. All O rings, gaskets, packings and mechanical seal renewed. Pump tried out and found to be in working condition. ","2024-02-16T23:59:09.999","","Completed","2024-02-14T23:59:09.999","No","No","No","Internal"]
[null,null,null,31692,69208,"55_Thu Aug 24 2023 00:27:07 GMT+0800","2024-02-20T23:59:09.999","Breakdown,Defect","Ship Staff","Ship Staff Insp.","Leak Noticed from Top End of Actuator for Draught Gauge Valve Port Side ","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","","","","","Leak Rectified. ","2024-05-19T23:59:09.999","","Completed","2024-04-11T23:59:09.999","No","No","No","Internal","Has the vessel raised RO for this item? "]
[null,null,null,36411,36253,"0_Sat Jun 01 2024 17:44:14 GMT+0800","2024-02-23T23:59:09.999","Observation","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","Chain blocks in Engine room monthly inventory list and the actual list of blocks were not coinciding .","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","8.50","Medium","",""," Chain blocks which were  taken on deck  brought back  to engine room, after which the  inventory list and actual number of chain block found to be matching as per the the list.",null,"","Completed","2024-02-23T23:59:09.999","No","No","No","External"]
[null,null,null,36412,96387,"0_Sat Jun 01 2024 17:46:15 GMT+0800","2024-02-23T23:59:09.999","Observation","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","1 SCBA set in fire control station low pressure warning whistle was defective.","LSA / FFA","Safety / LSA / FFA","Equipment Related","8.70","Medium","","","Defective whistle replaced with new one.",null,"","Completed","2024-02-23T23:59:09.999","No","No","No","External"]
[null,null,null,36415,32220,"0_Sat Jun 01 2024 17:49:59 GMT+0800","2024-02-23T23:59:09.999","Observation","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","Pumproom 2nd Deck AUS Pump guard was not extending fully protected and exposed 33 cms","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.46","Very High","",""," Pumproom 2nd Deck AUS Pump guard  fabricated and put in place , now it is fully protected.",null,"","Completed","2024-02-27T23:59:09.999","No","No","No","External"]
[null,null,null,34481,86414,"55_Fri Mar 01 2024 20:33:25 GMT+0800","2024-02-23T23:59:09.999","Observation","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","The two horizontal motor shafts of the AUS vacuum pump unit installed on the second deck at the top of the pump room were not completely provided with safety guards, and the each rotary shaft was approximately 35cm exposed.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","5.11","Low","",""," Protection covers have been fabricated on board and installed to completely shield the exposed shaft sections of both the horizontal motor shafts of the AUS vacuum pump units.\nAll other pump shafts were checked onboard and found to be adequately covered with safety guards.\n\n\n","2024-03-23T23:59:09.999","","Completed","2024-02-27T23:59:09.999","No","No","No","External"]
[null,null,null,34482,84084,"55_Fri Mar 01 2024 20:37:08 GMT+0800","2024-02-23T23:59:09.999","Observation","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","Low air pressure alarming device (whistle type) of a SCBA set located in the fire control station was defective and not activated alarming sound when tested. (The whistling device of the SCBA was loose and removing easily, if fixed it firmly then not activating alarming sound when tested.)","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.43","High","","","We wish to confirm that the SCBA Set whistle was aligned correctly and the Allen bolt adequately tightened during the inspection and the same rectified prior inspector’s disembarkation. The SCBA set whistle was tested multiple times and found to be in good working order. \n\nAll other SCBA set whistles and other components were checked for tightness and found to be in order.\n","2024-03-23T23:59:09.999","","Completed","2024-02-27T23:59:09.999","No","No","No","External"]
[null,null,null,35712,80556,"55_Wed May 22 2024 18:29:41 GMT+0800","2024-02-25T23:59:09.999","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","NEW BRIDGE SPLIT AC TO BE INSTALLED ","Accommodation","Navigation","Equipment Related","","","","","NEW BRIDGE SPLIT AC INSTALLED","2024-07-01T23:59:09.999","","Completed","2024-05-07T23:59:09.999","No","No","No","Internal"]
[null,null,null,38480,58981,"55_Mon Jan 06 2025 20:57:33 GMT+0800","2024-02-28T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","The cladding on the EGB has been wasted at various locations near HP and Superheater header leading to leakage of exhaust gas during sailing. \n","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","","","",""," Hot work carried out after office concurrence , new lagging and cladding material fitted. no leak observed.\n","2024-05-01T23:59:09.999","","Completed","2024-04-19T23:59:09.999","No","No","No","Internal"]
[null,null,null,34473,36472,"55_Wed Feb 28 2024 07:12:52 GMT+0800","2024-02-28T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","Pin hole at 2 locations on 2 pipe sections which is below the water line in ballast condition in Galley Overboard Pipeline. ","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","New valve fitted, Fabrication of pipe to be carried out. Pipe changed, job completed","2024-05-16T23:59:09.999","","Completed","2024-04-06T23:59:09.999","No","No","No","Internal"]
[null,null,null,34474,71033,"55_Wed Feb 28 2024 07:22:01 GMT+0800","2024-02-28T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","The cladding on the EGB has been wasted at various locations near HP and Superheater header leading to leakage of exhaust gas during sailing. ","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","",""," Hot work carried out after office concurrence , new lagging and cladding material fitted. no leak observed.","2024-05-01T23:59:09.999","","Completed","2024-04-19T23:59:09.999","No","No","No","Internal"]
[null,null,null,34476,91895,"55_Sat Mar 02 2024 11:00:27 GMT+0800","2024-03-01T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","Both LO purifier heaters Temperature Controller is erractic","E/R - Purifier","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Presently the purifier temperature  controller adjusted & is working satisfactory.  LO purifier heaters cleaned and now working satisfactory","2024-05-16T23:59:09.999","","Completed","2024-05-15T23:59:09.999","No","No","No","Internal"]
[null,null,null,35412,46970,"55_Sun Mar 31 2024 21:05:30 GMT+0800","2024-04-01T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","IG ISLOATION VALVE ( NO. IG 43) NOT SHUTTING FULLY (100%)","Inert Gas","Cargo / Ballast Systems","Equipment Related","8.23","Medium","","","Seatring renewed and IG Isolation valve (NO. IG 43) operating fully in open and close position. ","2024-07-01T23:59:09.999","","Completed","2024-05-07T23:59:09.999","No","No","No","Internal"]
[null,null,null,35416,95245,"55_Tue Apr 23 2024 07:15:09 GMT+0800","2024-04-07T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","Flow failure alarm  in Fixed gas ballast detection system & spaces ","Miscellaneous","Cargo / Ballast Systems","Equipment Related","5.21","Medium","","","Service technician attended the vessel in April 2024.  Pumproom fixed gas detection system was giving frequent fault alarm of Analyser Pump Failure. Troubleshooting carried out and now the system is working normal.  For Ballast tanks Will check the trueness in laden passage, right now all the ballast tanks are full & there is no alarm in the system","2024-07-07T23:59:09.999","","Completed","2024-06-22T23:59:09.999","No","No","No","Internal"]
[null,null,null,35414,26451,"55_Tue Apr 09 2024 08:07:26 GMT+0800","2024-04-08T23:59:09.999","Observation","Ship Staff","Ship Staff Insp.","Pin hole on outlet water spool piece of EGCS pump A.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","EGCS Pump A isolated, and valves shut ,New spool piece fabricated and fitted on discharge side, ","2024-06-16T23:59:09.999","","Completed","2024-05-30T23:59:09.999","No","No","No","Internal"]
[null,null,null,35703,93859,"55_Tue May 21 2024 17:33:11 GMT+0800","2024-04-25T23:59:09.999","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","STBD SIDE FWD NO1 RAMP BEND TO RECTIFIED","Deck - Pipe / Fittings","General Appearance","External Factors","11.1","High","","","Job Completed- Rectified","2024-06-25T23:59:09.999","","Completed","2024-06-11T23:59:09.999","No","No","No","Internal"]
[null,null,null,35705,14192,"55_Tue May 21 2024 20:44:39 GMT+0800","2024-04-25T23:59:09.999","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","PV BREAKER SIGHT GLASS TO BE RENEWED.","Inert Gas","Cargo / Ballast Systems","External Factors","8.7","High","","","Renewed","2024-07-25T23:59:09.999","","Completed","2024-06-23T23:59:09.999","No","No","No","Internal"]
[null,null,null,35706,90317,"55_Tue May 21 2024 20:48:26 GMT+0800","2024-04-25T23:59:09.999","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","MOORING WINCHES BRANCH HYDRAULIC LINES TO BE RENEWED.","Deck - Mooring Machinery","Mooring","External Factors","11.4","Very High","","","Various sections for Hydraulic lines renewed.","2024-07-25T23:59:09.999","","Completed","2024-06-11T23:59:09.999","No","No","No","Internal"]
[null,null,null,35707,64493,"55_Tue May 21 2024 20:50:36 GMT+0800","2024-04-25T23:59:09.999","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","DERUSTING OF WINCHES AND HYDRAULIC LINES TO BE CARRIED OUT.","Deck - Mooring Machinery","Mooring","External Factors","11.4","Very High","","","Derusting of winches and hydraulic lines connected to it completed.","2024-06-25T23:59:09.999","","Completed","2024-06-06T23:59:09.999","No","No","No","Internal"]
[null,null,null,35708,53542,"55_Tue May 21 2024 20:55:51 GMT+0800","2024-04-25T23:59:09.999","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","GANGWAY SPARE MOTORS IN MIDSHIP LOCKER TO BE OVERHAULED AND MADE OPERATIONAL, IF REQUIRED SPARE TO BE ORDERED.","Deck - Machinery","Safety / LSA / FFA","Equipment Related","5.47","Medium","","","Gangway spare motor overhauled & kept as spare","2024-07-25T23:59:09.999","","Completed","2024-07-11T23:59:09.999","No","No","No","Internal"]
[null,null,null,35709,25555,"55_Tue May 21 2024 20:29:47 GMT+0800","2024-04-25T23:59:09.999","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","FOAM MONITOR NUMBERING TO BE RENEWED.","LSA / FFA","Safety / LSA / FFA","Human Error","5.35","Medium","","","FOAM MONITOR NUMBERING RENEWED","2024-05-25T23:59:09.999","","Completed","2024-05-11T23:59:09.999","No","No","No","Internal"]
[null,null,null,35710,62089,"55_Tue May 21 2024 20:59:17 GMT+0800","2024-04-25T23:59:09.999","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","VRCS HIGH PRESSURE SETTING TO BE ADJUSTED AND PRESSURE SURGE TO BE INVESTIGATE AND RECTIFIED","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","Trouble shooting carried out. Unloader spool spindle cleaned and fit back, found working satisfactory","2024-07-25T23:59:09.999","","Completed","2024-05-30T23:59:09.999","No","No","No","Internal"]
[null,null,null,36403,66120,"0_Sat Jun 01 2024 16:24:45 GMT+0800","2024-04-26T23:59:09.999","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Leak from EGCS sample water analysing cabinet to be rectified","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.11","Medium","","","water leak was on the line of turbidity sensor line rectified ","2024-08-31T23:59:09.999","","Completed","2024-06-21T23:59:09.999","No","No","No","Internal"]
[null,null,null,36407,37099,"55_Sat Jun 01 2024 16:20:40 GMT+0800","2024-04-26T23:59:09.999","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","DG2 Exhaust manifold has leak stains, leak to be identified and rectified","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","",""," DG2 Exhaust manifold  leak Rectified.","2024-05-21T23:59:09.999","","Completed","2024-05-21T23:59:09.999","No","No","No","Internal"]
[null,null,null,36408,33156,"0_Sat Jun 01 2024 16:34:36 GMT+0800","2024-04-26T23:59:09.999","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Lube oil drums to be secured with 3 nos of bulldog grips with wooden plank between the wire ropes and the oil drums","Miscellaneous","Eng. / Strg. Comp.","Behaviour Based","","","","","Additional wire clip fitted on wire ropes with wooden plank between wire ropes and LO drums",null,"","Completed","2024-05-21T23:59:09.999","No","No","No","Internal"]
[null,null,null,36420,85539,"0_Sat Jun 01 2024 16:32:11 GMT+0800","2024-04-26T23:59:09.999","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Soot leak from Maine engine T/C exhaust Bypass valve to identified and rectified","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Leak rectified","2024-06-01T23:59:09.999","","Completed","2024-05-21T23:59:09.999","No","No","No","Internal"]
[null,null,null,36421,25115,"0_Sat Jun 01 2024 16:28:16 GMT+0800","2024-04-26T23:59:09.999","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Sea water leak from EGCS inlet analyser pH container leak.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.11","Medium","","","Container renewed & leak rectified\n","2024-08-01T23:59:09.999","SSUN240066","Completed","2024-06-29T23:59:09.999","No","No","No","Internal"]
[null,null,null,35704,92032,"55_Tue May 21 2024 20:34:51 GMT+0800","2024-04-26T23:59:09.999","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","IG  BRANCH LINE VALVES TO BE DERUSTED AND GREASED.","Inert Gas","Cargo / Ballast Systems","External Factors","8.50","Medium","","","IG BRANCH VALVES & LINES DERUSTING & PAINTING COMPLETED. VALVES GREASING COMPLETED.","2024-07-26T23:59:09.999","","Completed","2024-06-28T23:59:09.999","No","No","No","Internal"]
[null,null,null,34475,15287,"55_Wed Feb 28 2024 07:24:04 GMT+0800","2024-04-27T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","The pH sensor water container has a pin hole on the top cover.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.11","Medium","","","Spares received & container renewed","2024-07-01T23:59:09.999","SSUN240066","Completed","2024-07-04T23:59:09.999","No","No","Yes","Internal"]
[null,null,null,35418,60730,"55_Wed May 15 2024 20:52:24 GMT+0800","2024-05-14T23:59:09.999","Observation,Breakdown","Ship Staff","Ship Staff Insp.","WHRS Hp circulating pump #2 not developing sufficient pressure .","E/R - Boiler,E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.6","Very High","","","Found #1 Hp pump discharge valve not holding and water passing to the suction line of #1 hp pump. same rectified by changing dischrage side non return valve on other pump.","2024-08-01T23:59:09.999","RO SSUN 240116 Raised for the same.","Completed","2024-06-08T23:59:09.999","No","No","No","Internal"]
[null,null,null,35711,72946,"55_Thu May 30 2024 13:45:53 GMT+0800","2024-05-21T23:59:09.999","Critical Equipment","Ship Staff","Ship Staff Insp.","Oily water separtor Discharge pump and Aeration Pump seal Leaking","Critical Equip.","MARPOL Related","Equipment Related","10.32","Very High","","","After office concurrence,  Under Job order number V-SSUN041957-24  ,Oily Water Separator  Discharge pump and Aeration pump seal renewed , same tried out, working  satisfactory. office informed of the same.","2024-05-26T23:59:09.999","","Completed","2024-05-25T23:59:09.999","No","No","No","Internal"]
[null,null,null,26778,39736,"55_Mon Sep 12 2022 14:27:41 GMT+0800","2024-05-30T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","Various electrical panels in vessel without indications, due faulty indicator lamp unit and faulty winding heater timer","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","11.10","Medium","","","The indication lamps are faulty and hence raised required spares. \nAll indication lamps are now working ","2024-07-01T23:59:09.999","SSUN230018","Completed","2024-06-02T23:59:09.999","No","No","No","Internal","Spares will be supplied in Singapore "]
[null,null,null,36404,29849,"55_Mon Jun 10 2024 15:03:43 GMT+0800","2024-06-07T23:59:09.999","Defect,Observation","Ship Staff","Ship Staff Insp.","Inlet water analyzer turbidity sensor faulty, found water leakage inside sensor.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","RO raised for the same, Tried to rectify fault by changing O rings on water chamber of turbidity sensor but after some period water leak started again. We have started inlet water analyser other sensors by bypassing turbidity sensor. Vessel received new Turbidity sensor and installed on inlet analyser, Turbidity sensor configured for inlet analyser. ","2024-09-07T23:59:09.999","SSUN 240133","Completed","2024-08-29T23:59:09.999","No","No","No","Internal","Noted shall try to connect the spares at earliest opportunity. "]
[null,null,null,38478,14432,"55_Mon Jan 06 2025 20:55:14 GMT+0800","2024-06-07T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","Inlet water analyzer turbidity sensor faulty, found water leakage inside sensor.\n","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","RO raised for the same, Tried to rectify fault by changing O rings on water chamber of turbidity sensor but after some period water leak started again. We have started inlet water analyser other sensors by bypassing turbidity sensor. Vessel received new Turbidity sensor and installed on inlet analyser, Turbidity sensor configured for inlet analyser. \n","2024-09-07T23:59:09.999","","Completed","2024-08-29T23:59:09.999","No","No","No","Internal"]
[null,null,null,36394,22856,"55_Mon Jun 10 2024 14:58:40 GMT+0800","2024-06-11T23:59:09.999","Observation","Ship Staff","Ship Staff Insp.","GE Lub oil purifier bottom bearing cover leaking.","E/R - Purifier","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","waiting for spares. Spares received and job completed. ","2024-08-01T23:59:09.999","SSUN240108","Completed","2024-06-11T23:59:09.999","No","No","No","Internal"]
[null,null,null,36395,87215,"55_Wed Jun 12 2024 12:32:02 GMT+0800","2024-06-13T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","pressure switch MP55 on provision referigirating compressor #1 is faulty. Giving erratic output.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","RO SSUN240129 raised for the pressure switch MP55., Vessel checked and rectified fault in pressure switch. Job completed.","2024-08-13T23:59:09.999","SSUN240129","Completed","2024-07-10T23:59:09.999","No","No","No","Internal"]
[null,null,null,39976,null,"55_Fri Mar 21 2025 02:13:16 GMT+0000","2024-06-14T23:59:09.999","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","EMERGENCY GENERATOR ROOM CONDUIT ACCESS WAS NOTED HOLED WITH THE COVER MISSING.","Miscellaneous","General Appearance","Equipment Related","","","","","Permanent repair carried out. Defect deffered to DD","2024-09-19T23:59:09.999","","Completed","2024-09-14T23:59:09.999","No","No","No","Internal"]
[null,null,null,36396,27227,"55_Mon Jun 24 2024 12:59:25 GMT+0800","2024-06-14T23:59:09.999","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Pumproom Damper Door Hinges to be freed & lubricated","Miscellaneous","General Appearance","Equipment Related","","","","","FREED & LUBRICATED","2024-07-13T23:59:09.999","","Completed","2024-06-24T23:59:09.999","No","No","No","Internal"]
[null,null,null,36397,71052,"55_Mon Jun 24 2024 13:37:26 GMT+0800","2024-06-14T23:59:09.999","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","VALVES ON DECK AIR LINE ARE LEAKING","Deck - Pipe / Fittings","General Appearance","Equipment Related","","","","","Leaking valves renewed.","2024-09-14T23:59:09.999","","Completed","2024-07-13T23:59:09.999","No","No","No","Internal"]
[null,null,null,36398,29925,"55_Mon Jun 24 2024 13:41:30 GMT+0800","2024-06-14T23:59:09.999","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","GENERAL CORROSION NOTED ON PIPELINES ONBOARD (FWD/AFT & ATHWARTSHIP) ESPECIALLY AT THE U CLAMPS","Deck - Pipe / Fittings","General Appearance","Inappropriate Procedure","","","","","DERUSTING & PAINTING OF OVERHEAD DECK PIPELINES Completed. PLEASE REFER WEEKLY DECK MAINTENANCE REPORT","2024-09-14T23:59:09.999","","Completed","2024-07-13T23:59:09.999","No","No","No","Internal"]
[null,null,null,36399,23593,"55_Mon Jun 24 2024 14:08:38 GMT+0800","2024-06-14T23:59:09.999","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","VESSEL PROVIDED WITH INFLATABLE PFD; NO TEST OR SERVICING RECORDS AVAILABLE","LSA / FFA","Safety / LSA / FFA","Inappropriate Procedure","","","","","SIX MONTHLY INSPECTION IS AVAILABLE IN PMS PAL.  ALSO THE LIFEVEST RECIEVED IN OCT 2023. ONE YEAR SERVICING IS RECOMMENDED BY THE MANUFACTURER BY SELF ONBOARD.  MONTHLY CHECKS FOR PFD IS ALSO AVAILABLE IN PAL UNDER 3OFF DISCIPLINE. SERVICING & INSPECTION WILL BE CARRIED OUT ONCE DUE.","2024-09-14T23:59:09.999","","Completed","2024-06-27T23:59:09.999","No","No","No","Internal"]
[null,null,null,36401,27064,"55_Mon Jun 24 2024 13:39:02 GMT+0800","2024-06-14T23:59:09.999","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","VALVE WHEELS ON THE DECK AIR LINE & FRESH WATER LINE IN VERY POOR CONDITION","Deck - Pipe / Fittings","General Appearance","Equipment Related","","","","","VALVE WHEELS RENEWED","2024-09-14T23:59:09.999","","Completed","2024-07-16T23:59:09.999","No","No","No","Internal"]
[null,null,null,36402,65826,"55_Mon Jun 24 2024 13:33:35 GMT+0800","2024-06-14T23:59:09.999","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","RECIRCULATION VALVE ON THE HYDRAULIC LINES ON DECKNOT MARKED","Miscellaneous","General Appearance","Inappropriate Procedure","","","","","STENCILLING CARRIED OUT","2024-07-14T23:59:09.999","","Completed","2024-07-03T23:59:09.999","No","No","No","Internal"]
[null,null,null,36405,98413,"55_Mon Jun 24 2024 13:30:14 GMT+0800","2024-06-14T23:59:09.999","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","PV VALVE INSTALLED ON IG TO BALLAST LINE NOTED IN VERY POOR CONDITION","Inert Gas","General Appearance","Equipment Related","","","","","DERUSTIING & PAINTING COMPLETED, FLAME SCREEN RENEWED","2024-09-14T23:59:09.999","","Completed","2024-06-29T23:59:09.999","No","No","No","Internal"]
[null,null,null,36406,71783,"55_Mon Jun 24 2024 13:35:14 GMT+0800","2024-06-14T23:59:09.999","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","MARKINGS ON SOUNDING PORTS MISSING","Miscellaneous","General Appearance","Inappropriate Procedure","","","","","STENCILLING & HIGHLIGHTING COMPLETED","2024-07-14T23:59:09.999","","Completed","2024-07-02T23:59:09.999","No","No","No","Internal"]
[null,null,null,36414,64560,"55_Mon Jun 24 2024 13:17:51 GMT+0800","2024-06-14T23:59:09.999","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","PV Breaker Sight glass with slight Cracked & level not readable.","Inert Gas","Cargo / Ballast Systems","Equipment Related","","","","","Sight glass Renewed. Liquid topped up. In This type of PV Breaker we cannot see the lvel of liquid above 400mmWG","2024-07-13T23:59:09.999","","Completed","2024-06-23T23:59:09.999","No","No","No","Internal"]
[null,null,null,36416,63092,"55_Mon Jun 24 2024 13:45:00 GMT+0800","2024-06-14T23:59:09.999","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","CHAIN BLOCK IN MIDSHIP STORE NOTED WITH DAMAGED SAFETY LATCH","Miscellaneous","Safety / LSA / FFA","Inappropriate Procedure","","","","","CHAIN BLOCK IN USE DISCARDED, AS ITS CHAIN ALSO FOUND IN POOR CONDITION","2024-07-14T23:59:09.999","","Completed","2024-06-22T23:59:09.999","No","No","No","Internal"]
[null,null,null,36417,69616,"55_Mon Jun 24 2024 14:10:44 GMT+0800","2024-06-14T23:59:09.999","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","SAAB SCU SCREEN NOT OPERATIONAL","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","RECTIFIED, CHECKED &  WORKING SATISFACTORY","2024-09-14T23:59:09.999","","Completed","2024-06-19T23:59:09.999","No","No","No","Internal"]
[null,null,null,36418,29147,"55_Mon Jun 24 2024 13:28:04 GMT+0800","2024-06-14T23:59:09.999","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","FWD ROPE STORE COVER NOT CLOSING","Deck - Pipe / Fittings","General Appearance","Inappropriate Procedure","","","","","Rope store cover  Freeing completed. Now the the cover is closing properly.","2024-07-14T23:59:09.999","","Completed","2024-06-25T23:59:09.999","No","No","No","Internal"]
[null,null,null,36419,74611,"55_Mon Jun 24 2024 13:26:02 GMT+0800","2024-06-14T23:59:09.999","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ISC SPANNERS IN ISC BOX NOT ACCESSIBLE / STUCK TO THE BOX","LSA / FFA","Safety / LSA / FFA","Inappropriate Procedure","","","","","SPANNERS WERE STUCK WITH PAINT. CLEARED & GREASED","2024-06-24T23:59:09.999","","Completed","2024-06-22T23:59:09.999","No","No","No","Internal"]
[null,null,null,38418,12909,"55_Wed Jan 08 2025 21:14:12 GMT+0800","2024-08-21T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","IG SYSTEM O2 ANALYZER SENSOR FOR NO#2 RESPONSE IS VERY SLOW AND CALIBRATION IS DIFFICULT AS IT TAKES LONG TIME TO GET CORRECT OXYGEN READING.\n","Elect. Mach. & Equip.","Safety / LSA / FFA","Equipment Related","","","","","IG SYSTEM O2 ANALYZER SENSOR FOR NO #2 REPLACED WITH NEW SENSOR. FOUND WORKING SATISFACTORY.","2024-10-31T23:59:09.999","","Completed","2025-02-06T23:59:09.999","No","No","No","Internal"]
[null,null,null,38457,66858,"55_Mon Jan 06 2025 20:36:14 GMT+0800","2024-09-02T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","VRCS Solenoid Valve for Unload on order\n","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","Unloading pressure switch & solenoid valve renewed, made operational.\n","2024-12-02T23:59:09.999","","Completed","2024-12-02T23:59:09.999","No","No","No","Internal"]
[null,null,null,38464,75219,"55_Mon Jan 06 2025 20:48:53 GMT+0800","2024-09-02T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","BWTS - BT 1211 Filter inlet valve Cannot operate Remotely from CCR\n","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","","","","","Troubleshooting carried out. All these valves are now opening from CCR and also on local mode. (Local mode is from valve control and not by manual hydraulic pump).\n","2024-12-02T23:59:09.999","","Completed","2024-09-05T23:59:09.999","No","No","No","Internal"]
[null,null,null,38476,39598,"55_Mon Jan 06 2025 20:50:57 GMT+0800","2024-09-02T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","BWTS - BT 2213 Filter bypass valve cannot operate remotely from CCR. \n","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","","","","","Troubleshooting carried out. All these valves are now opening from CCR and also on local mode. (Local mode is from valve control and not by manual hydraulic pump).\n","2024-12-02T23:59:09.999","","Completed","2024-09-05T23:59:09.999","No","No","No","Internal"]
[null,null,null,38477,76329,"55_Mon Jan 06 2025 20:52:56 GMT+0800","2024-09-02T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","BWTS- BT 2211 Filter inlet valve cannot operate remotely from CCR\n","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","","","","","Troubleshooting carried out. All these valves are now opening from CCR and also on local mode. (Local mode is from valve control and not by manual hydraulic pump).\n","2024-12-02T23:59:09.999","","Completed","2024-09-05T23:59:09.999","No","No","No","Internal"]
[null,null,null,37545,19423,"55_Sat Sep 07 2024 00:06:02 GMT+0800","2024-09-02T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","Port side Pilot Ladder is overdue for renewal\n","Miscellaneous","ISM Related","External Factors","5.47","Medium","","","New pilot ladder received and old one renewed.","2024-12-02T23:59:09.999","SSUN240151\n","Completed","2024-11-16T23:59:09.999","No","No","No","Internal"]
[null,null,null,37548,51603,"55_Sat Sep 07 2024 00:12:05 GMT+0800","2024-09-02T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","BWTS Electrolyser water level sensor Not working. level switch LS 1111 monitors water level after electrolyser \n","Elect. Mach. & Equip.","Cargo / Ballast Systems","Equipment Related","6.21","High","","","Level switch received through RO - SSUN240131 & renewed. Found working satisfactory.\n","2024-12-02T23:59:09.999","SSUN240131\n","Completed",null,"No","No","No","Internal"]
[null,null,null,37549,56587,"55_Sat Sep 07 2024 00:03:01 GMT+0800","2024-09-02T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","VRCS Solenoid Valve for Unload on order\n","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","Unloading pressure switch & solenoid valve renewed, made operational.\n","2024-12-02T23:59:09.999","SSUN240128\n","Completed","2024-12-02T23:59:09.999","No","No","No","Internal"]
[null,null,null,37564,18701,"55_Fri Sep 06 2024 21:09:04 GMT+0800","2024-09-02T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","BWTS- BT 2211 Filter inlet valve cannot operate remotely from CCR\n","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","6.21","High","","","Troubleshooting carried out. All these valves are now opening from CCR and also on local mode. (Local mode is from valve control and not by manual hydraulic pump).","2024-12-02T23:59:09.999","","Completed","2024-09-05T23:59:09.999","No","No","No","Internal"]
[null,null,null,37565,81220,"55_Fri Sep 06 2024 21:16:53 GMT+0800","2024-09-02T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","BWTS - BT 2213 Filter bypass valve cannot operate remotely from CCR. \n","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","6.21","High","","","Troubleshooting carried out. All these valves are now opening from CCR and also on local mode. (Local mode is from valve control and not by manual hydraulic pump).","2024-12-02T23:59:09.999","","Completed","2024-09-05T23:59:09.999","No","No","No","Internal"]
[null,null,null,37566,39803,"55_Fri Sep 06 2024 21:18:07 GMT+0800","2024-09-02T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","BWTS - BT 1211 Filter inlet valve Cannot operate Remotely from CCR","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","6.21","High","","","Troubleshooting carried out. All these valves are now opening from CCR and also on local mode. (Local mode is from valve control and not by manual hydraulic pump).","2024-12-02T23:59:09.999","","Completed","2024-09-05T23:59:09.999","No","No","No","Internal"]
[null,null,null,37567,34913,"55_Sun Sep 15 2024 20:03:29 GMT+0800","2024-09-02T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","Chemcal locker door -  rubber packing sealing lips/Channel found wasted ","Miscellaneous","ISM Related","Equipment Related","5.2","Very High","","","Fabricated & Renewed","2024-12-02T23:59:09.999","","Completed","2024-09-08T23:59:09.999","No","No","No","Internal"]
[null,null,null,37568,60646,"55_Sat Sep 07 2024 00:00:50 GMT+0800","2024-09-02T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","Port windlass direction control valve for heave and lower is leaking\n","Deck - Mooring Machinery","Mooring","Equipment Related","","","","","During Both Operations in Corpus chrsiti, no leaks were found.","2024-12-02T23:59:09.999","SSUN230199\n","Completed","2024-09-25T23:59:09.999","No","No","No","Internal"]
[null,null,null,37569,76181,"55_Fri Sep 06 2024 23:58:45 GMT+0800","2024-09-02T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","Port & Stbd Windlass Brake cylinder seal is leaking\n","Deck - Mooring Machinery","Mooring","Equipment Related","","","","","No leaks as of now. Both the Brake cylinders are working satisfactory","2024-12-02T23:59:09.999","SSUN230199\n","Completed","2024-09-25T23:59:09.999","No","No","No","Internal"]
[null,null,null,37575,85166,"55_Tue Oct 01 2024 09:28:10 GMT+0800","2024-09-03T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","AUX ENGINE FUEL OIL VISCOTHERM SHOWING WRONG TEMPERATURES CORRESPONDING TO VISCOSITY INDEX THUS NEEDED CALIBRATION AND CLEANING OF SENSOR ","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","AUX ENGINE VISCOTHERM MADE OPERATIONAL","2024-12-02T23:59:09.999","","Completed","2024-09-28T23:59:09.999","No","No","No","Internal"]
[null,null,null,37570,77407,"55_Sun Sep 15 2024 20:08:59 GMT+0800","2024-09-04T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","Engine Room davit Wire drum found wasted & Holed","Miscellaneous","General Appearance","Equipment Related","","","","","Wasted portion repaired by hot work & made operational.","2024-12-03T23:59:09.999","","Completed","2024-09-17T23:59:09.999","No","No","No","Internal"]
[null,null,null,38415,40310,"55_Wed Jan 08 2025 21:10:48 GMT+0800","2024-09-07T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","# 1 FWG salinometer found not working.\n","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","RO SSUN240180 raised, spare received & salinometer renewed. \n",null,"","Completed","2025-01-23T23:59:09.999","No","No","No","Internal"]
[null,null,null,38458,40625,"55_Mon Jan 06 2025 20:32:43 GMT+0800","2024-09-11T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","Both L/B bilge pumps diaphragm found damaged.\n","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","New bilge pumps received and old ones renewed.\n","2024-12-11T23:59:09.999","","Completed","2024-11-17T23:59:09.999","No","No","No","Internal"]
[null,null,null,38285,94995,"55_Thu Oct 17 2024 17:31:42 GMT+0800","2024-09-11T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","Both L/B bilge pumps diaphragm found damaged.","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","New bilge pumps received and old ones renewed.","2024-12-11T23:59:09.999","","Completed","2024-12-12T23:59:09.999","No","No","No","Internal"]
[null,null,null,37577,37227,"55_Tue Oct 01 2024 02:23:51 GMT+0800","2024-09-11T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","Wire drum of Engine room davit found wasted & Holed","Miscellaneous","General Appearance","Equipment Related","","","","","Fabricated & renewed","2024-11-10T23:59:09.999","","Completed","2024-09-17T23:59:09.999","No","No","No","Internal"]
[null,null,null,38423,80084,"55_Wed Jan 08 2025 21:18:09 GMT+0800","2024-09-12T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","EGCS INLET ANALYZER TURBIDITY SENSOR GONE FAULTY AS INTERNAL LEAK GAVE WIRE BREAK ALARM. TURBIDITY SENSOR NEED REPLACEMENT.\n","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","THIS TURBIDITY SENSOR REPLACED WITH NEW SPARE. THE READING IS BEING SHOWN ON THE LOCAL MONITOR OF WATER INLET ANALYSER, HOWEVER THE SAME IS NOT GETTING DISPLAYED ON THE HMI IN THE ECR. OFFICE HELP SOUGHT","2024-12-31T23:59:09.999","","Completed","2025-02-08T23:59:09.999","No","No","No","Internal"]
[null,null,null,37555,48686,"55_Sun Sep 15 2024 04:10:09 GMT+0800","2024-09-12T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","WHEN EGCS PUMPS STOPS IN BALLAST CONDITION BOTH SEAWATER FEED PUMP NON RETURN VALVES LEAK PASS FROM DISCHARGE SIDE TO SUCTION SIDE, NON RETURN VALVES ARE NOT HOLDING AND DUE TO THIS DISCHRGE LINE GOES UNDER HUGE VIBRATIONS. THESE VIBRATION CAN CAUSE DAMAGE TO PUMPS, INLET ANALYZER, PRESSURE SWITCHES ETC. ","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.31","Very High","","","EGCS PUMPS NON RETURN VALVES NEEDS REPLACEMENT, NEW NON RETURN VALVES NEED TO ORDER AND REPLACE ONCE RECEIVE, MEAN TIME AS SOON AS WE STOP EGCS  PUMPS WE HAVE TO SHUT SEA WATER PUMP DISCHARGE VALVES AND INLET ANALYZER SAMPLING VALVES. VLAVES RECEIVED THROUGH RO - SSUN240240 & RENEWED.","2025-01-01T23:59:09.999","","Completed","2024-12-04T23:59:09.999","No","No","No","Internal"]
[null,null,null,38462,33221,"55_Mon Jan 06 2025 20:43:38 GMT+0800","2024-09-14T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","OWS ALARM BACK UP ON COMPUTER IS NOT POSSIBLE AS ALL COMPUTERS ARE LOCK AND NEW EXTERNAL PROGRAM CANNOT RUN ON ECR COMPUTER\n","Elect. Mach. & Equip.","MARPOL Related","Equipment Related","","","","","OWS alarm back up was taken with personal laptop.\n","2024-10-01T23:59:09.999","","Completed","2024-09-14T23:59:09.999","No","No","No","Internal"]
[null,null,null,37572,26148,"55_Sun Sep 15 2024 04:24:59 GMT+0800","2024-09-14T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","OWS ALARM BACK UP ON COMPUTER IS NOT POSSIBLE AS ALL COMPUTERS ARE LOCK AND NEW EXTERNAL PROGRAM CANNOT RUN ON ECR COMPUTER","Elect. Mach. & Equip.","MARPOL Related","Equipment Related","10.37","Medium","","","OWS alarm back up was taken with personal laptop.","2024-10-01T23:59:09.999","","Completed","2024-09-17T23:59:09.999","No","No","No","Internal"]
[null,null,null,38463,66307,"55_Mon Jan 06 2025 20:46:16 GMT+0800","2024-09-17T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","Aux D/G governor found malfunctioning\n","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Aux D/G governor renewed with spare governor.\n","2024-09-17T23:59:09.999","","Completed","2024-09-17T23:59:09.999","No","No","No","Internal"]
[null,null,null,37574,38051,"0_Mon Sep 30 2024 02:39:33 GMT+0800","2024-09-17T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","Aux D/G governor found malfuntioning","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Aux D/G governor renewed with spare governor.","2024-09-17T23:59:09.999","","Completed","2024-09-17T23:59:09.999","No","No","No","Internal"]
[null,null,null,37573,72652,"0_Mon Sep 30 2024 02:46:33 GMT+0800","2024-09-18T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","VRCS valve indicator OT 135 found malfunctioning ","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","VRCS faulty valve indicator  OT 135 renewed & tested. Found working satisfactory.","2024-10-01T23:59:09.999","","Completed","2024-09-18T23:59:09.999","No","No","No","Internal"]
[null,null,null,37576,89042,"55_Thu Sep 26 2024 20:32:48 GMT+0800","2024-09-26T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","EGCS Pressure transmitter - PT 2020A ( 0 ~ 4 bar ) on Jet section found malfunctioning.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","PT 2020A ( 0 ~ 4 bar ) replaced with a new spare & found working satisfactory.","2024-09-26T23:59:09.999","","Completed","2024-09-26T23:59:09.999","No","No","No","Internal"]
[null,null,null,37571,18627,"55_Mon Sep 30 2024 03:26:23 GMT+0800","2024-09-28T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","Dairy room fan found making noise.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","Dairy room fan renewed & made operational.","2024-12-27T23:59:09.999","","Completed","2024-09-28T23:59:09.999","No","No","No","Internal"]
[null,null,null,38461,45412,"55_Mon Jan 06 2025 20:41:08 GMT+0800","2024-10-01T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","# 2 FWG salinometer control unit PCB found damaged.\n","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","The salinometer control unit is interchanged from # 1 FWG & made operational.\n","2024-12-31T23:59:09.999","","Completed","2024-10-01T23:59:09.999","No","No","No","Internal"]
[null,null,null,37578,74268,"55_Mon Sep 30 2024 02:31:35 GMT+0800","2024-10-01T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","# 2 FWG salinometer control unit PCB found damaged.\n","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","The salinometer control unit is interchanged from # 1 FWG & made operational.","2024-12-31T23:59:09.999","","Completed","2024-10-01T23:59:09.999","No","No","No","Internal"]
[null,null,null,38263,23704,"55_Thu Oct 17 2024 16:03:51 GMT+0800","2024-10-02T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","Emergency Generator room Door - rubber packing sealing lips/Channel found wasted & holed","Miscellaneous","ISM Related","Equipment Related","5.20","Medium","","","Fabricated & renewed.","2024-11-02T23:59:09.999","","Completed","2024-10-06T23:59:09.999","No","No","No","Internal"]
[null,null,null,38264,59822,"55_Thu Oct 17 2024 16:15:19 GMT+0800","2024-10-02T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","E/R duct flaps found wasted(3 no's).  ","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","All 3 duct flaps fabricated & fitted. Made operational.","2025-01-01T23:59:09.999","","Completed","2024-10-06T23:59:09.999","No","No","No","Internal"]
[null,null,null,39336,71893,"0_Mon Feb 10 2025 08:32:08 GMT+0800","2024-10-02T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","Aux D/G T/C mounting block holding down bolt threads found damaged","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Aux D/G T/C mounting block  holding down bolts new threads were made. RO-SSUN240248- received, T/C mounting block replaced with new spare.","2025-01-02T23:59:09.999","RO-SSUN240248","Completed","2025-02-04T23:59:09.999","No","No","No","Internal"]
[null,null,null,38277,31167,"0_Thu Oct 17 2024 17:49:29 GMT+0800","2024-10-06T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","Upper deck (S) accommodation gas detection sensor triggering sensor fault alarm","Elect. Mach. & Equip.","Safety / LSA / FFA","Equipment Related","","","","","Sensor calibrated as per makers procedure, sensor found working normal after the calibration. Alarm tried out, found working satisfactory.","2024-11-01T23:59:09.999","","Completed","2024-10-25T23:59:09.999","No","No","No","Internal"]
[null,null,null,38274,62713,"0_Thu Oct 17 2024 16:21:13 GMT+0800","2024-10-08T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","Emergency generator room door found wasted at few places.","Miscellaneous","Structural Condn. / WT integrity ","Equipment Related","","","","","Repaired by removing wasted portion & welding new plate. ","2024-10-08T23:59:09.999","","Completed","2024-10-08T23:59:09.999","No","No","No","Internal"]
[null,null,null,38419,98492,"55_Wed Jan 08 2025 21:09:48 GMT+0800","2024-10-09T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","OWS 3-way valve is leaking through spindle gland.\n","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","3-way valve to spindle gland packing & o - ring renewed. No leak observed.","2025-01-08T23:59:09.999","","Completed","2025-01-31T23:59:09.999","No","No","No","Internal"]
[null,null,null,38265,85090,"0_Thu Oct 17 2024 16:25:10 GMT+0800","2024-10-09T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","OWS 3-way overboard valve actuator air found leaking from the actuator shaft.","Critical Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","Actuator overhauled, O -ring on actuator shaft renewed. Actuator made operational.","2024-10-09T23:59:09.999","","Completed","2024-10-09T23:59:09.999","No","No","No","Internal"]
[null,null,null,38269,32646,"0_Thu Oct 17 2024 16:29:17 GMT+0800","2024-10-09T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","LP dosing pump tripped","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","","","","","Pump removed, found diaphragm leaking.  Same renewed, pump made operational.","2024-11-01T23:59:09.999","","Completed","2024-10-09T23:59:09.999","No","No","No","Internal"]
[null,null,null,38266,32610,"55_Thu Oct 17 2024 17:57:32 GMT+0800","2024-10-11T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","Fish room fan motor, found making noise.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","Fish room fan motor replaced with o'hauled one. ","2024-11-01T23:59:09.999","","Completed","2024-10-11T23:59:09.999","No","No","No","Internal"]
[null,null,null,38273,33999,"55_Thu Oct 17 2024 18:21:12 GMT+0800","2024-10-11T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","ME servo rail securing clamps (2 no's) found broken.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","ME servo rail securing clamps (2 no's) fabricated & fitted.","2024-11-01T23:59:09.999","","Completed","2024-10-12T23:59:09.999","No","No","No","Internal"]
[null,null,null,38268,19121,"0_Thu Oct 17 2024 16:48:18 GMT+0800","2024-10-12T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","ME auto backwash filter found leaking through the spindle bore on the cover. ","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","O-ring found damaged, same renewed.","2024-11-01T23:59:09.999","","Completed","2024-10-12T23:59:09.999","No","No","No","Internal"]
[null,null,null,38284,42208,"0_Thu Oct 17 2024 18:10:51 GMT+0800","2024-10-13T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","Port side bridge wing telephone found defective.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","Port side bridge wing defective telephone renewed.","2024-11-01T23:59:09.999","","Completed","2024-10-13T23:59:09.999","No","No","No","Internal"]
[null,null,null,38267,74000,"0_Thu Oct 17 2024 17:21:04 GMT+0800","2024-10-14T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","STBD L/B engine not starting on # 2 Battery.","LSA / FFA","Emgcy. Systems","Equipment Related","","","","","STBD L/B both batteries, renewed. L/B tested, found working satisfactory.","2024-11-01T23:59:09.999","","Completed","2024-10-17T23:59:09.999","No","No","No","Internal"]
[null,null,null,38410,39932,"55_Wed Jan 08 2025 20:47:41 GMT+0800","2024-10-16T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","VECS O2 sensor is malfunctioning,\n","Cargo Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","RO - SSUN240201 received, same replaced & calibrated. Found working satisfactory.\n","2025-01-16T23:59:09.999","","Completed","2025-02-04T23:59:09.999","No","No","No","Internal"]
[null,null,null,38416,57587,"55_Wed Jan 08 2025 21:07:03 GMT+0800","2024-10-16T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","ME # 4 Unit cylinder pressure transmitter is faulty.\n","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","RO-SSUN240094 raised, spare received. The fault was found with loose connection, same tightened. Found working satisfactory.\n","2025-01-16T23:59:09.999","","Completed","2025-01-21T23:59:09.999","No","No","No","Internal"]
[null,null,null,38449,31795,"55_Wed Jan 08 2025 20:49:39 GMT+0800","2024-10-16T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","# 1 Control air dryer is in-operational\n","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","Replaced # 1 Control air dryer with new spare. Tried out, found working satisfactory.\n","2025-01-16T23:59:09.999","","Completed","2025-02-14T23:59:09.999","No","No","No","Internal"]
[null,null,null,38450,34001,"55_Wed Jan 08 2025 20:57:46 GMT+0800","2024-10-16T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","AUX Boiler UNISAB controller display is not visible,\n","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","RO-SSUN240062 received, display renewed. working satisfactory.\n","2025-01-16T23:59:09.999","","Completed","2024-12-26T23:59:09.999","No","No","No","Internal"]
[null,null,null,38451,56576,"55_Wed Jan 08 2025 20:56:01 GMT+0800","2024-10-16T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","# 2 IG O2 sensor is malfunctioning,\n","Inert Gas","Eng. / Strg. Comp.","Equipment Related","","","","","RO-SSUN240176 is on order, faulty new sensors(2 no's) were received. Supplier supplied 2 sensors on GC, same renewed & found working satisfactory.\n","2025-01-16T23:59:09.999","","Completed","2025-02-06T23:59:09.999","No","No","No","Internal"]
[null,null,null,38467,97847,"55_Wed Jan 08 2025 21:00:24 GMT+0800","2024-10-16T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","\"Galley overboard pipe has a soft patch. Require renewal.\t\"\n","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","\"Galley overboard pipe renewed by fabricating new pipe.\t","2025-01-16T23:59:09.999","","Completed","2024-12-18T23:59:09.999","No","No","No","Internal"]
[null,null,null,38272,25907,"55_Sat Oct 19 2024 03:31:30 GMT+0800","2024-10-16T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","OWS flocculant chamber body has  crack,","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","",""," Cold work carried out.","2025-01-16T23:59:09.999","","Completed","2024-10-17T23:59:09.999","No","No","No","Internal"]
[null,null,null,38279,69503,"0_Sat Oct 19 2024 03:24:29 GMT+0800","2024-10-16T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","E/R atmospheric oil mist detection system # 3 sensor for D/G's is not working, ","LSA / FFA","Eng. / Strg. Comp.","Equipment Related","","","","","Sensor renewed, system put back in to operation.","2025-01-16T23:59:09.999","","Completed","2024-12-11T23:59:09.999","No","No","No","Internal"]
[null,null,null,38460,55323,"55_Mon Jan 06 2025 20:38:51 GMT+0800","2024-10-17T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","Ows flocculant chamber has a crack\n","Critical Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","Cold work carried out, leak rectified.\n","2024-10-17T23:59:09.999","","Completed","2024-10-17T23:59:09.999","No","No","No","Internal"]
[null,null,null,38270,30833,"0_Thu Oct 17 2024 18:07:12 GMT+0800","2024-10-17T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","Found minor crack on OWS flocculant chamber ","Critical Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","Cold work carried out, leak rectified.","2025-01-16T23:59:09.999","","Completed","2024-10-17T23:59:09.999","No","No","No","Internal"]
[null,null,null,38291,83537,"0_Mon Dec 16 2024 09:43:43 GMT+0800","2024-10-17T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","Engine room vent fan #2 tripped on restarting. ","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","Opened up motor terminal box for inspection, noted all cables intact & in order. Checked further & noted defective overload relay. O/L relay renewed with new spare. Fan tried out and noted working in good order.\t\t\t\t\t\t\t\t\t\t\t\t\n","2024-12-17T23:59:09.999","","Completed","2024-10-17T23:59:09.999","No","No","No","Internal"]
[null,null,null,38271,91128,"55_Mon Oct 28 2024 01:05:18 GMT+0800","2024-10-20T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","Exhaust Gas leakage found through # 1 D/G T/C turbine side casing.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","DG 1 TC EXHAUST GAS LEAKAGE RECTIFIED BY RENEWING DAMAGED STUDS IN THE TURBINE SIDE CASING.","2024-11-01T23:59:09.999","","Completed","2024-10-22T23:59:09.999","No","No","No","Internal"]
[null,null,null,38276,43076,"55_Mon Oct 28 2024 01:09:22 GMT+0800","2024-10-20T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","Engine room vent fan #2 tripped, found not starting. ","Elect. Mach. & Equip.","Emgcy. Systems","Equipment Related","","","","","The Engine room vent fan #2 tripping due to defective overload relay. O/L relay renewed with new spare. Fan tried out and noted working in good order.\t\t\t\t\t\t\t\t\t\t\t\t\n","2024-11-01T23:59:09.999","","Completed","2024-10-20T23:59:09.999","No","No","No","Internal"]
[null,null,null,38278,98871,"55_Mon Oct 28 2024 01:13:30 GMT+0800","2024-10-23T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","OIL SEEPAGE OBSERVED THROUGH SERVICE AIR COMPRESSOR IST STAGE LINER . ","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related","","","","","SERVICE AIR COMPRESSOR IST STAGE LINER REMOVED,  OIL SEEPAGE RECTIFIED BY CLEANING & APPLYING HIGH TEMP SILICON.","2024-11-01T23:59:09.999","","Completed","2024-10-23T23:59:09.999","No","No","No","Internal"]
[null,null,null,38286,52347,"0_Mon Dec 16 2024 09:50:46 GMT+0800","2024-10-24T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","EMG DIESEL GENERATOR EXHAUST PIPE FOUND WASTED","Deck - Pipe / Fittings","Emgcy. Systems","Equipment Related","","","","","PIPE REMOVED AND FABRICATED NEW IN E/R WORKSHOP. \n","2025-01-01T23:59:09.999","","Completed","2024-10-24T23:59:09.999","No","No","No","Internal"]
[null,null,null,38275,36532,"55_Mon Oct 28 2024 01:17:02 GMT+0800","2024-10-25T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","EMG DIESEL GENERATOR EXHAUST PIPE FOUND WASTED, ","Miscellaneous","Emgcy. Systems","Equipment Related","","","","","EMG DIESEL GENERATOR EXHAUST PIPE REMOVED AND FABRICATED NEW IN E/R WORKSHOP. \n","2025-01-25T23:59:09.999","","Completed","2024-10-27T23:59:09.999","No","No","No","Internal"]
[null,null,null,38280,86612,"55_Sat Oct 19 2024 03:28:24 GMT+0800","2024-10-25T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","Found telephone handset cable damaged for auto telephone in Emergency generator room .","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","Renewed telephone handset cable for auto telephone in Emergency generator room. Checked the communication between emergency generator room and wheel house / ECR with auto telephone . Noted in good order.","2025-01-25T23:59:09.999","","Completed","2024-10-25T23:59:09.999","No","No","No","Internal"]
[null,null,null,38289,93011,"0_Mon Dec 16 2024 09:58:36 GMT+0800","2024-10-29T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","AFT HYD PUMP MOTOR SPIDER COUPLING FOUND BROKEN.","Deck - Mooring Machinery","Eng. / Strg. Comp.","Equipment Related","","","","","  SPIDER COUPLING RENEWED.",null,"","Completed","2024-10-29T23:59:09.999","No","No","No","Internal"]
[null,null,null,38290,96884,"0_Mon Dec 16 2024 10:00:35 GMT+0800","2024-10-30T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","M6 MOORING WINCH PLATFORM FOUND WASTED.\n","Miscellaneous","General Appearance","Equipment Related","","","","","MOORING WINCH PLATFORM REPAIR WORK CARRIED OUT.\n","2025-01-01T23:59:09.999","","Completed",null,"No","No","No","Internal"]
[null,null,null,38292,74382,"0_Mon Dec 16 2024 10:03:05 GMT+0800","2024-10-31T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","AUX BOILER # 2 WATER LEVEL CONTROLLER POSITIONER FOUND NOT WORKING. ","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","AUX BOILER # 2 WATER LEVEL CONTROLLER POSITIONER RENEWED.","2025-01-01T23:59:09.999","","Completed","2024-10-31T23:59:09.999","No","No","No","Internal"]
[null,null,null,38293,40030,"0_Mon Dec 16 2024 10:05:51 GMT+0800","2024-10-31T23:59:09.999","Defect","Ship Staff","Ship Staff Insp."," Jet assist system for Aux D/G found non-operational.\t\t\t\t\t\t\t\t\t\t\n","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Aux D/G jet assist system solenoid renewed. Operation of the jet assist solenoid checked and confirmed working in good order.\t\t\t\t\t\t\t\t\t\t\t\t\n","2025-01-01T23:59:09.999","","Completed","2024-10-31T23:59:09.999","No","No","No","Internal"]
[null,null,null,38300,55793,"0_Mon Dec 16 2024 10:09:28 GMT+0800","2024-11-01T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","EMG GENERATOR CO2 CABINET (OUTSIDE EMG D/G ROOM)  DOOR HINGES FOUND WASTED, \n","LSA / FFA","Emgcy. Systems","Equipment Related","","","","","CO2 CABINET (OUTSIDE EMG D/G ROOM)  DOOR HINGES RENEWED.","2025-01-01T23:59:09.999","","Completed","2024-11-01T23:59:09.999","No","No","No","Internal"]
[null,null,null,38459,71330,"55_Mon Jan 06 2025 20:29:09 GMT+0800","2024-11-15T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","# 2 Filter fault for BWTS system got triggered & were unable to start BWTs system\n","Miscellaneous","Cargo / Ballast Systems","Equipment Related","","","","","# 2 Filter fault for BWTS system rectified by lifting the filter cover, checking for any obstructions for the filter. checking the operation of the motor by separating it from the filter assembly. Put back the filter cover properly in place and tried out motor. Noted OK.\n","2025-01-01T23:59:09.999","","Completed","2024-11-16T23:59:09.999","No","No","No","Internal"]
[null,null,null,38294,76823,"0_Mon Dec 16 2024 10:18:00 GMT+0800","2024-11-15T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","# 2 Filter fault for BWTS system got triggered & were unable to start BWTs system","Miscellaneous","Cargo / Ballast Systems","Equipment Related","","","","","# 2 Filter fault for BWTS system rectified by lifting the fliter cover, checking for any obstructioins for the filter. checking the operation of the motor by seperating it from the filter assembly. Put back the filter cover properly in place and tried out motor. Noted OK.\t\t\t\t\t\t\t\t\t\t\t\t\n","2025-01-01T23:59:09.999","","Completed","2024-11-16T23:59:09.999","No","No","No","Internal"]
[null,null,null,38296,57251,"55_Mon Dec 16 2024 09:41:33 GMT+0800","2024-11-15T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","Window wiper ( Center ) not working.\t\t\t\t\t\t\t\t\t\t\t\t\n","Elect. Mach. & Equip.","Navigation","Equipment Related","","","","","Removed the fitting from its location & noted springs and belt broken in place. Renewed both the springs and the belt. Tried out, found working satisfactory.\t\t\t\n","2025-01-01T23:59:09.999","","Completed","2024-11-15T23:59:09.999","No","No","No","Internal"]
[null,null,null,38409,25757,"55_Wed Jan 08 2025 20:41:04 GMT+0800","2024-11-21T23:59:09.999","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Port lifeboat window glass is hazy and needs to be cleaned and if not possible to clean then order for new glass.\n","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","RO - SSUN240271 raised, new window glass received and renewed.\n","2024-12-21T23:59:09.999","SSUN240271\n","Completed","2025-02-07T23:59:09.999","No","No","No","Internal"]
[null,null,null,38433,17407,"55_Wed Jan 08 2025 20:35:04 GMT+0800","2024-11-21T23:59:09.999","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ER store cave to be arranged. Suggest all items are removed, store cleaned and arranged.\n","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","Arrangment done\n","2024-12-21T23:59:09.999","","Completed","2025-01-16T23:59:09.999","No","No","No","Internal"]
[null,null,null,38468,99040,"55_Wed Jan 08 2025 20:43:01 GMT+0800","2024-11-21T23:59:09.999","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Port side HFO manifold presentation flange bolts to be renewed.\n","Deck - Pipe / Fittings","General Appearance","Equipment Related","","","","","Bolts renewed.\n","2025-01-01T23:59:09.999","","Completed","2024-12-18T23:59:09.999","No","No","No","Internal"]
[null,null,null,38469,43698,"55_Wed Jan 08 2025 20:38:37 GMT+0800","2024-11-21T23:59:09.999","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Grey water tank vent head has a crack. To be repaired\n","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Grey water tank vent head crack repaired.\n","2025-01-01T23:59:09.999","","Completed","2024-12-17T23:59:09.999","No","No","No","Internal"]
[null,null,null,38470,31702,"55_Wed Jan 08 2025 20:36:55 GMT+0800","2024-11-21T23:59:09.999","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Galley drain overboard line found with soft patch. Line to be renewed.\n","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Pipe renewed.\n","2024-12-21T23:59:09.999","","Completed","2024-12-18T23:59:09.999","No","No","No","Internal"]
[null,null,null,38245,12986,"0_Sun Dec 15 2024 16:06:39 GMT+0800","2024-11-21T23:59:09.999","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","M6 mooring winch brake is not properly installed and was found improperly seated on the brake band. To be removed and new brake to be installed. \t","Deck - Machinery","Mooring","Equipment Related","","","","","M6 mooring winch brake alignment adjusted without changing the brake setting. Winch tried out. Found working satisfactorily.","2024-12-21T23:59:09.999","","Completed","2024-12-17T23:59:09.999","No","No","No","Internal"]
[null,null,null,38246,15546,"55_Sun Dec 15 2024 16:02:18 GMT+0800","2024-11-21T23:59:09.999","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Port lifeboat window glass is hazy and needs to be cleaned and if not possible to clean then order for new glass.","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","Window glass renewed with spare glass onboard. RO raised for spare.","2024-12-21T23:59:09.999","SSUN240271","Completed","2024-01-26T23:59:09.999","No","No","No","Internal","noted , awaiting vendor supply."]
[null,null,null,38247,26724,"0_Sun Dec 15 2024 16:22:09 GMT+0800","2024-11-21T23:59:09.999","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Galley drain overboard line found with soft patch. Line to be renewed. \t","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Pipe renewed","2024-12-21T23:59:09.999","","Completed","2024-11-16T23:59:09.999","No","No","No","Internal"]
[null,null,null,38248,72085,"0_Sun Dec 15 2024 16:10:52 GMT+0800","2024-11-21T23:59:09.999","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Starboard Provision crane goose neck found wasted. To be renewed. ","Deck - Machinery","General Appearance","Equipment Related","","","","","Crane goose neck repaired.","2024-12-21T23:59:09.999","","Completed","2024-12-15T23:59:09.999","No","No","No","Internal"]
[null,null,null,38249,97174,"0_Sun Dec 15 2024 16:05:26 GMT+0800","2024-11-21T23:59:09.999","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Ship staff not familiar with requirement for 2 safety valves for the BA compressor for Lifeboat bottle and SCBA bottles. Safety valve available onboard. Training to be imparted to all to ensure proper implementation. ","Miscellaneous","Safety / LSA / FFA","Knowledge Based","","","","","Training imparted to all officers and crew members",null,"","Completed","2024-12-15T23:59:09.999","No","No","No","Internal"]
[null,null,null,38250,41181,"0_Sun Dec 15 2024 16:03:41 GMT+0800","2024-11-21T23:59:09.999","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Grey water tank vent head has a crack. To be repaired","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Grey water tank vent head crack, repaired by hot work.","2025-01-01T23:59:09.999","","Completed","2024-12-31T23:59:09.999","No","No","No","Internal"]
[null,null,null,38252,41858,"0_Sun Dec 15 2024 16:25:17 GMT+0800","2024-11-21T23:59:09.999","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Port and Starboard manifold gratings to be derusted and painted. ","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Port and Starboard manifold gratings derusted and painted. ","2025-02-01T23:59:09.999","","Completed","2025-02-14T23:59:09.999","No","No","No","Internal"]
[null,null,null,38253,54820,"0_Sun Dec 15 2024 16:28:37 GMT+0800","2024-11-21T23:59:09.999","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ER store cave to be arranged. Suggest all items are removed, store cleaned and arranged. ","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","ER store cave  arranged","2024-12-21T23:59:09.999","","Completed","2024-12-20T23:59:09.999","No","No","No","Internal"]
[null,null,null,38254,41848,"0_Sun Dec 15 2024 16:16:18 GMT+0800","2024-11-21T23:59:09.999","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","MW2 gear oil found emulsified. Gear case to be inspected and oil to be renewed. Source of leak to be identified. ","Deck - Machinery","Mooring","Equipment Related","","","","","MW1 & MW2 gear oil renewed. Gear case inspected, found satisfactory.\nGauge glass cleaned.\n ","2024-12-21T23:59:09.999","","Completed","2024-12-17T23:59:09.999","No","No","No","Internal"]
[null,null,null,38255,62119,"0_Sun Dec 15 2024 16:18:05 GMT+0800","2024-11-21T23:59:09.999","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Bosun store davit hook safety latch found damaged. To be repaired. ","Deck - Pipe / Fittings","General Appearance","Equipment Related","","","","","Bosun store davit hook safety latch repaired. ","2024-11-28T23:59:09.999","","Completed","2024-12-06T23:59:09.999","No","No","No","Internal"]
[null,null,null,38256,26804,"0_Sun Dec 15 2024 16:23:38 GMT+0800","2024-11-21T23:59:09.999","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Anti-skid paint on the walkways on deck not very effective and needs to be redone. ","Miscellaneous","General Appearance","Equipment Related","","","","","Anti Skid paint applied on walkways, ramps and around mooring area","2025-01-01T23:59:09.999","","Completed","2024-12-13T23:59:09.999","No","No","No","Internal"]
[null,null,null,38258,33647,"0_Sun Dec 15 2024 16:29:51 GMT+0800","2024-11-21T23:59:09.999","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Fresh water generator no 1 not operational. Troubleshooting to be carried and to make it operational.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Will be done at the earliest.","2024-12-21T23:59:09.999","","Completed","2025-04-09T23:59:09.999","No","No","No","Internal","Defect is closed. As same was issued during MSI."]
[null,null,null,38261,60275,"55_Sun Dec 15 2024 15:53:26 GMT+0800","2024-11-21T23:59:09.999","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Port side HFO manifold presentation flange bolts to be renewed.","Deck - Pipe / Fittings","General Appearance","Equipment Related","","","","","Bolts  renewed.","2025-01-01T23:59:09.999","","Completed","2024-12-31T23:59:09.999","No","No","No","Internal"]
[null,null,null,38281,12274,"0_Sun Dec 15 2024 16:19:05 GMT+0800","2024-11-21T23:59:09.999","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Few lamp indicators for the remote hydraulic valves in the ER were found not working. Eg IG, IGG, High Sea Chest ","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Done","2024-12-06T23:59:09.999","","Completed","2024-12-06T23:59:09.999","No","No","No","Internal"]
[null,null,null,38282,78547,"0_Sun Dec 15 2024 16:09:33 GMT+0800","2024-11-21T23:59:09.999","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Securing hinge for the Fire box 23 on the poop peck to be derusted as condition found deteriorating. \t\t","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","Securing hinge attended & the defect rectified.","2024-12-21T23:59:09.999","","Completed","2024-12-11T23:59:09.999","No","No","No","Internal"]
[null,null,null,38283,84645,"0_Sun Dec 15 2024 16:12:56 GMT+0800","2024-11-21T23:59:09.999","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Greasing of all Boiler mounting valves to be carried out and several found dry. ","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","Both Aux Boiler mounting valves greasing carried out during Intermediate Boiler survey.","2024-12-06T23:59:09.999","","Completed","2024-11-22T23:59:09.999","No","No","No","Internal"]
[null,null,null,38287,30710,"0_Sun Dec 15 2024 16:20:43 GMT+0800","2024-11-21T23:59:09.999","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","EGCS Inlet WAU, pH sensor water pot found leaking. To be renewed. \t","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","\tEGCS Inlet WAU, pH sensor water pot found leaking.,same renewed. ","2024-12-06T23:59:09.999","","Completed","2024-12-02T23:59:09.999","No","No","No","Internal"]
[null,null,null,38295,76827,"0_Sun Dec 15 2024 16:27:32 GMT+0800","2024-11-21T23:59:09.999","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","High sea chest remote hydraulic valve in front of ECR found leaking. Leak to be repaired. ","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Leak repaired. ","2024-12-21T23:59:09.999","","Completed","2024-12-06T23:59:09.999","No","No","No","Internal"]
[null,null,null,40179,62111,"55_Sat Apr 12 2025 00:16:59 GMT+0800","2024-11-21T23:59:09.999","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Galley drain overboard line with soft patch, the same line to be renewed.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Pipe line renewed.","2024-12-21T23:59:09.999","","Completed","2024-11-21T23:59:09.999","No","No","No","Internal"]
[null,null,null,38298,63663,"0_Mon Dec 16 2024 10:24:43 GMT+0800","2024-11-27T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","ME UNIT NO 6 SECTION OF STARTING AIR LINE PIPE FOUND HOLED.\n","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","ME UNIT NO 6 SECTION OF STARTING AIR LINE PIPE REPLACED WITH NEW SPARE.\n","2025-01-01T23:59:09.999","","Completed","2024-11-27T23:59:09.999","No","No","No","Internal"]
[null,null,null,38407,17219,"55_Wed Jan 08 2025 20:29:14 GMT+0800","2024-12-02T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","IGS scrubber SW common manifold inlet to the nozzle sections are having pin holes.\n","Inert Gas","Eng. / Strg. Comp.","Equipment Related","","","","","All the pipe sections were removed & found heavily corroded, same were fabricated new.\nSystem tried out, found no leaks.","2025-03-01T23:59:09.999","","Completed","2025-01-14T23:59:09.999","No","No","No","Internal"]
[null,null,null,38454,33147,"55_Mon Jan 06 2025 20:19:06 GMT+0800","2024-12-02T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","IGS Scrubber tower floor found holed & fish plate found wasted.\n","Inert Gas","Eng. / Strg. Comp.","Equipment Related","","","","","Hot work carried out inside IGS Scrubber tower after receiving concurrence from office. Fish plate renewed and bottom holes filling carried out.\n","2025-01-01T23:59:09.999","","Completed","2024-12-22T23:59:09.999","No","No","No","Internal"]
[null,null,null,38262,59932,"55_Mon Dec 16 2024 19:42:52 GMT+0800","2024-12-02T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","IGS scrubber SW common manifold inlet to the nozzle sections are having pin holes.","Inert Gas","Eng. / Strg. Comp.","Equipment Related","","","","","Rectified by cold work","2025-03-01T23:59:09.999","","Completed","2025-01-02T23:59:09.999","No","No","No","Internal","Noted , plan the job at suitable anchorage."]
[null,null,null,38299,99841,"0_Mon Dec 16 2024 10:26:36 GMT+0800","2024-12-02T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","AUX BOILER MAIN FEED WATER PUMP NO 2 RECIRCULATION LINE FOUND LEAKING.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","MAIN FEED WATER PUMP NO 2 LEAKING RECIRCULATION LINE REMOVED FROM PLACE AND LEAK RECTIFIED BY WELDING IN WORKSHOP.","2025-01-01T23:59:09.999","","Completed","2024-12-02T23:59:09.999","No","No","No","Internal"]
[null,null,null,38303,93951,"55_Mon Dec 16 2024 10:35:51 GMT+0800","2024-12-02T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","IGS Scrubber tower floor found holed & fish plate found wasted.","Inert Gas","Eng. / Strg. Comp.","Equipment Related","","","","","Hot work carried out inside IGS Scrubber tower after receiving concurrence from office. Fish plate renewed and bottom holes filling carried out.\n","2025-01-01T23:59:09.999","","Completed","2024-12-03T23:59:09.999","No","No","No","Internal"]
[null,null,null,38305,93663,"0_Mon Dec 16 2024 10:48:15 GMT+0800","2024-12-02T23:59:09.999","Defect","Ship Staff","Ship Staff Insp."," BWTS level switch (EU - 1111 ) found malfunctioning.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","Renewed level switch (EU - 1111 ), new spare received for BWTS. Level alarm and function test satisfactory.\n","2025-01-01T23:59:09.999","","Completed","2024-12-02T23:59:09.999","No","No","No","Internal"]
[null,null,null,38301,87238,"0_Mon Dec 16 2024 10:29:07 GMT+0800","2024-12-03T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","Found lance redrawn proximity sensor for # 1 Aux Boiler damaged.  ","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","Renewed the damaged lance redrawn proximity sensor for # 1 Aux Boiler. ","2025-01-01T23:59:09.999","","Completed","2024-12-03T23:59:09.999","No","No","No","Internal"]
[null,null,null,38304,18112,"0_Mon Dec 16 2024 10:37:48 GMT+0800","2024-12-04T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","M.E. F.O. pump fuel leak off chamber found holed. ","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","M.E. F.O. pump fuel leak off chamber removed from place and leak rectified by welding in workshop. All working satisfactorily","2025-01-01T23:59:09.999","","Completed","2024-12-04T23:59:09.999","No","No","No","Internal"]
[null,null,null,38306,45100,"0_Mon Dec 16 2024 10:41:04 GMT+0800","2024-12-04T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","EGCS SW pump #1 discharge line stub piece flange sealing surface found wasted, s","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","EGCS SW pump #1 discharge line stub piece removed and  repair work was carried out by welding in workshop. EGCS SW pump #1 tried out, found working satisfactory.","2025-01-01T23:59:09.999","","Completed","2024-12-04T23:59:09.999","No","No","No","Internal"]
[null,null,null,38309,64049,"0_Mon Dec 16 2024 10:54:36 GMT+0800","2024-12-04T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","LSFO (P) bunker tank steam heating common return line gasket found leaking in Purifier room . ","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","LSFO (P) bunker tank steam heating common return line gasket renewed.","2025-01-01T23:59:09.999","","Completed","2024-12-04T23:59:09.999","No","No","No","Internal"]
[null,null,null,38456,67377,"55_Mon Jan 06 2025 20:25:40 GMT+0800","2024-12-05T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","Two holes found in EGCS scrubber jet section vertical ladder top leg.\n","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","The holes were repaired by coldwork. \n","2025-01-01T23:59:09.999","","Completed","2024-12-05T23:59:09.999","No","No","No","Internal"]
[null,null,null,38307,10027,"0_Mon Dec 16 2024 10:44:25 GMT+0800","2024-12-05T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.",". Two holes found in EGCS scrubber jet section vertical ladder top leg.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","The holes were repaired by coldwork. \n","2025-01-01T23:59:09.999","","Completed","2024-12-05T23:59:09.999","No","No","No","Internal"]
[null,null,null,38471,99941,"55_Tue Jan 14 2025 22:46:36 GMT+0800","2024-12-11T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","M5 mooring winch LP side hydraulic pipe found wasted.","Deck - Mooring Machinery","Eng. / Strg. Comp.","Equipment Related","","","","","M5 mooring winch LP side hydraulic pipe renewed by fabrication.","2025-01-01T23:59:09.999","","Completed","2024-12-12T23:59:09.999","No","No","No","Internal"]
[null,null,null,38302,92178,"0_Mon Dec 16 2024 11:00:08 GMT+0800","2024-12-11T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","FWD HYDRAULIC LO COOLER SW INLET PIPE FOUND LEAKING.","Deck - Pipe / Fittings","Mooring","Equipment Related","","","","","LEAKING SECTION OF FWD HYDRAULIC LO COOLER SW INLET PIPE FARICATED IN WORKSHOP.\n","2025-01-01T23:59:09.999","","Completed","2024-12-11T23:59:09.999","No","No","No","Internal"]
[null,null,null,38308,88087,"0_Mon Dec 16 2024 11:03:00 GMT+0800","2024-12-12T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","Aux DG giving random false alarms.\n","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","Suspected these alarms are  originating from the Main control unit. Replaced Main control & speed measuring unit with spare. Found working satisfactory.\n","2025-01-01T23:59:09.999","","Completed","2024-12-12T23:59:09.999","No","No","No","Internal"]
[null,null,null,38472,90683,"55_Tue Jan 14 2025 22:49:05 GMT+0800","2024-12-13T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","FWD Hydraulic Power Pack unit LO SW inlet pipe found leaking","Deck - Machinery","Eng. / Strg. Comp.","Equipment Related","","","","","FWD Hydraulic Power Pack unit LO SW inlet pipe renewed by fabrication. ","2025-01-01T23:59:09.999","","Completed","2024-12-14T23:59:09.999","No","No","No","Internal"]
[null,null,null,38297,36338,"0_Mon Dec 16 2024 10:58:11 GMT+0800","2024-12-13T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","HYDRAULIC DECK MACHINERY LOW PRESSURE LINE PIPE SECTION FOUND HOLED","Deck - Machinery","Mooring","Equipment Related","","","","","LEAKING SECTION OF HYDRAULIC PIPE FOR DECK MACHINERY FABRICATED NEW IN WORKSHOP.\n","2025-01-01T23:59:09.999","","Completed","2024-12-13T23:59:09.999","No","No","No","Internal"]
[null,null,null,38473,87344,"55_Tue Jan 14 2025 23:07:19 GMT+0800","2024-12-21T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","WHRS H.P DRUM FEED WATER INLET & BYPASS VALVE GASKET FOUND LEAKING.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","WHRS H.P DRUM FEED WATER INLET & BYPASS VALVE LEAK RECTIFIED BY RENEWAL OF THE GASKETS.","2025-01-01T23:59:09.999","","Completed","2024-12-21T23:59:09.999","No","No","No","Internal"]
[null,null,null,38474,26857,"0_Tue Jan 14 2025 23:10:37 GMT+0800","2024-12-24T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","MAIN DG NO. 1 STARTING AIR PRESSURE REDUCING VALVE FOUND LEAKING","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","MAIN DG NO. 1 STARTING AIR PRESSURE REDUCING VALVE OVERHAULED & LEAKRECTIFIED.","2024-12-24T23:59:09.999","","Completed","2024-12-24T23:59:09.999","No","No","No","Internal"]
[null,null,null,38475,47473,"0_Tue Jan 14 2025 23:14:07 GMT+0800","2024-12-25T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","IGS SCRUBBER TOWER SW INLET MANIFOLD & INLET PIPES TO NOZZLE SECTIONS FOUND WASTED","Inert Gas","Eng. / Strg. Comp.","Equipment Related","","","","","IGS SCRUBBER TOWER SW INLET MANIFOLD & INLET TO NOZZLE SECTIONS WASTED PIPES FABRICATED NEW","2024-12-30T23:59:09.999","","Completed","2024-12-29T23:59:09.999","No","No","No","Internal"]
[null,null,null,38483,40412,"0_Wed Jan 15 2025 23:26:26 GMT+0800","2024-12-27T23:59:09.999","Defect","Ship Staff","Ship Staff Insp."," F.O inlet temperature sensor for # 2 Diesel generator engine found defective. ","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Renewed the defective F.O inlet temperature sensor for # 2 Diesel generator engine. Tested the alarm and function. Noted working in good order after renewal.\n","2024-12-31T23:59:09.999","","Completed","2024-12-27T23:59:09.999","No","No","No","Internal"]
[null,null,null,38452,53459,"0_Sat Jan 04 2025 20:50:48 GMT+0800","2024-12-29T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","Noticed MSBD Low insulation on 220V distribution panel","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.24","Low","","","Deck light casing found damaged, same renewed.  220V low insulation alarm condition removed.","2025-01-06T23:59:09.999","","Completed","2025-01-04T23:59:09.999","No","No","No","Internal"]
[null,null,null,38455,69191,"55_Sat Dec 28 2024 14:45:51 GMT+0800","2024-12-29T23:59:09.999","Breakdown","Ship Staff","Ship Staff Insp.","AIS Transmission data has been reported to be missing by other passing ships and shore agencies ","Navigation - DGPS / EPFS / AIS","Navigation","Equipment Related","4.1","High","","","Arrangement of shore technician at Changxingdao made, AIS renewed.","2025-01-29T23:59:09.999","","Completed","2025-01-01T23:59:09.999","No","No","No","Internal"]
[null,null,null,38439,93490,"0_Wed Jan 15 2025 23:45:39 GMT+0800","2024-12-31T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","ME UNIT 2,3,4 & 5 JCW INLET& OUTLET VALVES ARE NOT HOLDING","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","SPARE VALVES ARE AVAILABLE, AWATING FOR OPPORTUNITY.","2025-02-01T23:59:09.999","","Completed","2025-01-21T23:59:09.999","No","No","No","Internal"]
[null,null,null,38453,83942,"55_Sat Jan 04 2025 20:45:43 GMT+0800","2024-12-31T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","T/G condenser cooling sea water pump found leaking from mechanical seal due to muddy water","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.31","Very High","","","T/G condenser cooling sea water pump leaky mechanical seal renewed.","2025-01-06T23:59:09.999","","Completed","2025-01-05T23:59:09.999","No","No","No","Internal"]
[null,null,null,38466,30002,"55_Mon Jan 06 2025 21:04:00 GMT+0800","2024-12-31T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","WHRS soot blow not possible from ECR panel.\n","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","Spares received and installed on by service engineer. System could not be tried out in presence of service engineer with ME stopped.System tried out at sea but found no response from ECR control as well as from local control panel. Communication with office and maker in progress. Presently, soot blow of EGB is carried out from local control panel. \n","2024-08-01T23:59:09.999","SSUN230029\n","Completed","2024-06-02T23:59:09.999","No","No","No","Internal"]
[null,null,null,38485,78433,"0_Wed Jan 15 2025 23:32:19 GMT+0800","2025-01-01T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","Observed JCW leak from # 1 D/G #2 unit cylinder head ","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","# 1 D/G #2 unit cylinder head replaced with reconditioned one, O-ring between Liner & cylinder head found damaged, same renewed.","2025-01-01T23:59:09.999","","Completed","2025-01-01T23:59:09.999","No","No","No","Internal"]
[null,null,null,40182,66890,"55_Sat Apr 12 2025 00:20:47 GMT+0800","2025-01-01T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","ME waste gate valve out let flange spectacle flange gasket found damaged","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","The gasket renewed.","2025-04-01T23:59:09.999","","Completed","2025-04-04T23:59:09.999","No","No","No","Internal"]
[null,null,null,38448,59754,"0_Thu Jan 16 2025 00:15:24 GMT+0800","2025-01-02T23:59:09.999","Defect","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","A low insulation of 1.6 megaohms was observed on the AC 220v feed panel located in the engine control room at the time of the inspection. It was reported that the low insulation was caused by the bad weather.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.24","Low","","","Trouble shooting is carried out.","2025-03-01T23:59:09.999","","Completed","2025-01-21T23:59:09.999","No","No","No","External"]
[null,null,null,38479,90604,"0_Wed Jan 15 2025 23:34:13 GMT+0800","2025-01-02T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","# 1 D/G HT CW pump seal found leaking through damaged mechanical seal.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","# 1 D/G HT CW pump replaced with a o'hauled one..","2025-01-02T23:59:09.999","","Completed","2025-01-02T23:59:09.999","No","No","No","Internal"]
[null,null,null,38486,63915,"55_Thu Jan 16 2025 00:09:44 GMT+0800","2025-01-02T23:59:09.999","Defect","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","The turbo generator condenser cooling seawater pump was permanently leaking drops of water from its mechanical seal at the time of the inspection. As reported by the chief engineer, the seal was damaged due to muddy water. ","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","The turbo generator condenser cooling seawater pump leaky mechanical seal renewed. ","2025-01-16T23:59:09.999","","Completed","2025-01-11T23:59:09.999","No","No","No","External"]
[null,null,null,38487,90560,"0_Thu Jan 16 2025 00:20:52 GMT+0800","2025-01-02T23:59:09.999","Defect","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","The nameplate showed that the maximum output voltage of the portable welding machine (Model: MMA-250L) located in the\nengine room workshop was 27.2V exceeding 25V.\n","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.37","Medium","","","Welding machine de-commissioned.","2025-01-06T23:59:09.999","","Completed","2025-01-03T23:59:09.999","No","No","No","External"]
[null,null,null,38437,41061,"55_Tue Jan 14 2025 12:49:48 GMT+0800","2025-01-03T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","Minor leak observed from No: 2 COP lower mechanical seal & oil seal.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","No: 2 COP lower oil seals & Mechanical seal renewed.","2025-02-15T23:59:09.999","","Completed","2025-02-20T23:59:09.999","No","No","No","Internal"]
[null,null,null,40180,38987,"55_Sat Apr 12 2025 00:25:00 GMT+0800","2025-01-04T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","NO.1 DG Turbocharger mounting block found crack and lube oil leak observed from the turbocharger base.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Mounting block and stud renewed with new spare. Holding down bolts renewed with new spares.","2025-04-01T23:59:09.999","","Completed","2025-04-04T23:59:09.999","No","No","No","Internal"]
[null,null,null,38482,19047,"0_Wed Jan 15 2025 23:42:58 GMT+0800","2025-01-07T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","MAIN AIR COMPRESSOR #1 COOLER INSPECTION CARRIED OUT. FOUND LEAK FROM ONE OF THE TUBES. ","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related","","","","","LEAK WAS RECTIFIED BY PUTTING A PLUG AND BOXED BACK. TRIED OUT FOUND SATISFACTORY.","2025-01-11T23:59:09.999","","Completed","2025-01-07T23:59:09.999","No","No","No","Internal"]
[null,null,null,38481,11460,"0_Wed Jan 15 2025 23:39:03 GMT+0800","2025-01-12T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","NO. 2 steering gear motor protection relay found malfunctioning.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","NO. 2 steering gear motor protection relay replaced with new one\t\t\t\t\t\t\t\t\t\t\t\t\n","2025-01-12T23:59:09.999","","Completed","2025-01-12T23:59:09.999","No","No","No","Internal"]
[null,null,null,38484,82325,"0_Wed Jan 15 2025 23:36:29 GMT+0800","2025-01-12T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","FO SLUDGE PUMP SECOND STAGE PINION GEAR FOUND BROKEN.\n","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","","","","","FO SLUDGE PUMP BROKEN SECOND STAGE PINION GEAR REPLACED WITH NEW SPARE.\n","2025-01-16T23:59:09.999","","Completed","2025-01-12T23:59:09.999","No","No","No","Internal"]
[null,null,null,38446,17113,"55_Wed Jan 15 2025 23:57:36 GMT+0800","2025-01-15T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","# 2 D/G EXHAUST VALVES FOUND BROKEN WHILE IN OPERATION, ALSO FOUND CYLINDER HEAD, PISTON, LINER, T/C & NOZZLE RING DAMAGED.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","CYLINDER HEAD, PISTON, LINER, T/C CARTRIDGE RENEWED, OLD NOZZLE RING FITTED . ","2025-01-17T23:59:09.999","","Completed","2025-01-19T23:59:09.999","No","No","No","Internal"]
[null,null,null,39327,36986,"55_Sun Feb 09 2025 09:55:26 GMT+0800","2025-01-15T23:59:09.999","Breakdown","Ship Staff","Ship Staff Insp.","# 1 D/G # 2 UNIT CYL HEAD EXH V/V FOUND BROKEN, SAME DAMAGED LINER, PISTON, CYL HEAD & T/C","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","# 1 D/G # 2 UNIT CYL HEAD, LINER, PISTON & T/C RENEWED.","2025-01-19T23:59:09.999","","Completed","2025-01-19T23:59:09.999","No","No","No","Internal"]
[null,null,null,39328,59333,"0_Sun Feb 09 2025 10:00:50 GMT+0800","2025-01-20T23:59:09.999","Breakdown","Ship Staff","Ship Staff Insp.","# 1 D/G # 4 UNIT CYL HEAD FOUND LEAKING WHILE BLOWING THROUGH DUE TO JCW LEAK FROM EXH VALVE SEAT","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","# 1 D/G # 4 UNIT CYL HEAD REPLACED WITH O'HAULED SPARE","2025-01-20T23:59:09.999","","Completed","2025-01-20T23:59:09.999","No","No","No","Internal"]
[null,null,null,39329,54245,"0_Sun Feb 09 2025 10:08:46 GMT+0800","2025-01-21T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","M.E. UNIT #2,3 & #4 JACKET WATER INLET AND OUTLET, # 5 UNIT INLET VALVES FOUND LEAKING\n","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","M.E. UNIT #2,3 & #4 JACKET WATER INLET AND OUTLET, # 5 UNIT INLET VALVE REPLACED WITH NEW SPARE.\n","2025-03-01T23:59:09.999","","Completed","2025-01-21T23:59:09.999","No","No","No","Internal"]
[null,null,null,39331,17334,"0_Sun Feb 09 2025 10:13:11 GMT+0800","2025-01-25T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","M.E. UNIT #2 ICU FOUND STUCK IN MAX POSITION.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","M.E. UNIT #2 ICU REPLACED WITH NEW SPARE. M.E. TRIED OUT. ALL FOUND SATISFACTORY.\n","2025-01-25T23:59:09.999","","Completed","2025-01-25T23:59:09.999","No","No","No","Internal"]
[null,null,null,39330,43950,"0_Sun Feb 09 2025 10:11:09 GMT+0800","2025-01-26T23:59:09.999","Defect","Ship Staff","Ship Staff Insp."," BWTS NEUTRALIZING LINE FOUND LEAKING","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","LEAKING BWTS NEUTRALIZING LINE RECTIFIED BY REPLACING LEAKING PIPE WITH NEW PIPE.","2025-03-01T23:59:09.999","","Completed","2025-01-26T23:59:09.999","No","No","No","Internal"]
[null,null,null,39332,87827,"0_Sun Feb 09 2025 10:22:04 GMT+0800","2025-01-26T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","NO 2 FWG EJECTOR PUMP MECHANICAL SEAL. FOUND LEAKING ","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","","","","","NO 2 FWG EJECTOR PUMP REPLACED WITH NEW MECHANICAL SEAL.. HOWEVER THE PUMP SAHFT THREADS FOUND DAMAGED, SAME RETHREADED WITH 2.5 PITCH THREAD & FITTED. ALSO MEXH SEAL COVER FOUND ERODED, SAME REPAURED WITH COLD WORK. NO LEAK OBSERVED. RO - SSUN250065 RAISED.\n","2025-03-01T23:59:09.999","RO - SSUN250065","Completed","2025-02-06T23:59:09.999","No","No","No","Internal"]
[null,null,null,39334,77168,"55_Sun Feb 09 2025 11:28:52 GMT+0800","2025-01-28T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","440V low insulation alarm getting activated frequently","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","440V low insulation rectified from Fish room evaporator fan motor.\t\t\t\t\t\t\t\t\t\t\t\t\n","2025-03-01T23:59:09.999","","Completed","2025-01-28T23:59:09.999","No","No","No","Internal"]
[null,null,null,39333,85028,"55_Sun Feb 09 2025 11:26:02 GMT+0800","2025-01-29T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","# 2 FWG discharge valve found leaking","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","# 2 FWG leaky discharge valve replaced with new spare.","2025-03-01T23:59:09.999","","Completed","2025-01-29T23:59:09.999","No","No","No","Internal"]
[null,null,null,39300,68944,"55_Sun Feb 09 2025 11:18:21 GMT+0800","2025-01-30T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","EGCS SW pump discharge common leaking through a hole of 10 mm dia.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","EGCS SW pump discharge manifold leakage rectified by welding a doubler plate on the hole.","2025-04-01T23:59:09.999","","Completed","2025-03-18T23:59:09.999","No","No","No","Internal"]
[null,null,null,39335,43481,"55_Sun Feb 09 2025 11:34:15 GMT+0800","2025-02-04T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","220 V  LOW INSULATION FOUND GETTING TRIGGERED.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","WHEEL HOUSE AC NOT WORKING UPON CHECKS FOUND 220V ALARM AND FOUND POWER CABLE FOR COMPRESSOR OUT DOOR UNIT BURNED REPAIRED CABLE AND FITTED BACK FOUND AC WORKING IN GOOD ORDER.\n","2025-03-01T23:59:09.999","","Completed","2025-02-04T23:59:09.999","No","No","No","Internal"]
[null,null,null,39348,38919,"55_Tue Feb 25 2025 14:15:15 GMT+0800","2025-02-07T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","No 3 Foam monitor valve found to be leaking.","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","Valve replaced with the spare valve available onboard","2025-03-07T23:59:09.999","","Completed","2025-03-01T23:59:09.999","No","No","No","Internal"]
[null,null,null,39340,78009,"0_Sun Feb 16 2025 16:48:21 GMT+0800","2025-02-13T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","WHEEL HOUSE WINDOW WIPER’S FOUND NOT WORKING.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","",""," FOUND BELT BROKEN SAME REPLACED AND TRIED OUT FOUND WORKING SATISFACTORY. \n","2025-05-13T23:59:09.999","","Completed","2025-02-13T23:59:09.999","No","No","No","Internal"]
[null,null,null,39342,40144,"55_Sun Feb 16 2025 16:56:13 GMT+0800","2025-02-13T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","BWTS RECTIFIER RF -142A STOP CONDITION SHOWING 10 A","E/R - Aux. Mach.","","","","","",""," AS PER OFFICE MAIL PCB INTER CHANGED WITH RESPECTED SETTINGS WITH RECTIFIER 142A AND 142B.  POST SWAPPING OF THE PCB'S ALL RECTIFIERS DISPLAY ARE SHOWING ZERO (0) AMPS IN STOP CONDITION.\n\n","2025-05-13T23:59:09.999","","Completed","2025-02-14T23:59:09.999","No","No","No","Internal"]
[null,null,null,39355,41215,"0_Sat Feb 15 2025 09:40:53 GMT+0800","2025-02-13T23:59:09.999","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Air leak form funnel flap air cylinder bellow.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Air leak form funnel flap air cylinder rectified.","2025-02-28T23:59:09.999","","Completed","2025-02-17T23:59:09.999","No","No","No","Internal"]
[null,null,null,39309,75351,"0_Sat Feb 15 2025 09:42:08 GMT+0800","2025-02-14T23:59:09.999","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","No.2 Aux boiler combustion air duct bellow is wrapped with canvas.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","# 2 Aux Boiler combustion air duct bellow replaced with new spare. ","2025-04-01T23:59:09.999","","Completed","2025-03-05T23:59:09.999","No","No","No","Internal","Pls plan to renew at next suitable opportunity."]
[null,null,null,39311,71502,"0_Sat Feb 15 2025 09:45:03 GMT+0800","2025-02-14T23:59:09.999","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","All flexible hoses to be identified and labelled as per MESQAC requirement.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","All flexible hoses to be identified and labelled as per MESQAC requirement & segregated","2025-03-26T23:59:09.999","","Completed","2025-03-05T23:59:09.999","No","No","No","Internal","Pls expedite."]
[null,null,null,39319,82961,"0_Sat Feb 15 2025 09:51:45 GMT+0800","2025-02-14T23:59:09.999","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Main and Aux engines leaks to be identified and rectified.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","All the leaks on Main and Aux engines leaks has been identified and rectified.","2025-03-26T23:59:09.999","","Completed","2025-03-14T23:59:09.999","No","No","No","Internal","Pls expedite."]
[null,null,null,39324,26988,"0_Sat Feb 15 2025 09:54:35 GMT+0800","2025-02-14T23:59:09.999","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Defective pressure gauges and thermometers on LT coolers to be renewed.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Defective pressure gauges and thermometers on LT coolers renewed.","2025-03-14T23:59:09.999","","Completed","2025-03-11T23:59:09.999","No","No","No","Internal","Pls check if vsl is having sufficient spares pressure gauges and create RO, if required."]
[null,null,null,39326,41061,"0_Sat Feb 15 2025 09:56:09 GMT+0800","2025-02-14T23:59:09.999","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Sea water leaks on # 1 FWG to be rectified.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","No fresh sea water leaks on # 1 FWG observed after cleaning the FWG.","2025-03-14T23:59:09.999","","Completed","2025-03-04T23:59:09.999","No","No","No","Internal","Identify the leaks and rectify."]
[null,null,null,39337,53324,"0_Sat Feb 15 2025 09:50:43 GMT+0800","2025-02-14T23:59:09.999","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Salt deposits and water marks on No.2 boiler casing to be cleaned and painted.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","Salt deposits and water marks on No.2 boiler casing cleaned and painted.","2025-03-14T23:59:09.999","","Completed","2025-02-14T23:59:09.999","No","No","No","Internal"]
[null,null,null,39338,97001,"0_Sat Feb 15 2025 10:00:05 GMT+0800","2025-02-14T23:59:09.999","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Both FWG salinometer cables are disconnected.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","# 1 FWG Salinometer renewed, # 2 FWG salinometer connections were renewed.","2025-02-28T23:59:09.999","","Completed","2025-01-29T23:59:09.999","No","No","No","Internal"]
[null,null,null,39339,20032,"0_Sat Feb 15 2025 09:43:46 GMT+0800","2025-02-14T23:59:09.999","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Incinerator W.O sett and serv. Tanks manhole covers to be covered with insulation lagging.","Hull & Tanks","Eng. / Strg. Comp.","Equipment Related","","","","","Incinerator W.O sett and serv. Tanks manhole covers covered with insulation lagging.","2025-02-28T23:59:09.999","","Completed","2025-02-16T23:59:09.999","No","No","No","Internal"]
[null,null,null,39341,68118,"0_Sun Feb 16 2025 16:50:46 GMT+0800","2025-02-14T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","ACCOMMODATION AIR CONDITIONER NO 2 DRIVING BELTS BROKEN.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","",""," BELTS REPLACED AND ADJUSTED TENSIONS ON BELTS AND STARTED AIR CON.  \n","2025-05-14T23:59:09.999","","Completed","2025-02-14T23:59:09.999","No","No","No","Internal"]
[null,null,null,39345,77499,"0_Sat Feb 15 2025 09:53:00 GMT+0800","2025-02-14T23:59:09.999","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Aux DG Unit no.4 cooling water outlet temperature gauge is defective.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Aux DG Unit no.4 cooling water outlet temperature defective gauge renewed.","2025-03-14T23:59:09.999","","Completed","2025-03-01T23:59:09.999","No","No","No","Internal"]
[null,null,null,39346,31739,"0_Sat Feb 15 2025 09:46:08 GMT+0800","2025-02-14T23:59:09.999","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Combustible materials and oil drums to be removed from the storage space in the 2nd deck port side adjacent to sludge collecting tank and space to be cleaned.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","Combustible materials and oil drums removed from the storage space in the 2nd deck port side adjacent to sludge collecting tank and space cleaned & painted.","2025-03-14T23:59:09.999","","Completed","2025-02-26T23:59:09.999","No","No","No","Internal"]
[null,null,null,39347,15347,"0_Sat Feb 15 2025 09:49:19 GMT+0800","2025-02-14T23:59:09.999","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Minor leaks in steering gear to be identified and rectified.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Minor leaks in steering gear identified and rectified.","2025-03-14T23:59:09.999","","Completed","2025-02-27T23:59:09.999","No","No","No","Internal"]
[null,null,null,39352,92067,"55_Thu Feb 13 2025 16:58:32 GMT+0800","2025-02-14T23:59:09.999","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Port lifeboat self-lowering wire handle is detached.","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","Self lowering wire of both lifeboats renewed with spare wire onboard.\nNew handles fabricated. As per design, Handles remains detached from the self lowering wire and is connected to wire in a quick release manner while self  wire lowering to be used. ","2025-03-01T23:59:09.999","","Completed","2025-03-01T23:59:09.999","No","No","No","Internal"]
[null,null,null,39356,37082,"55_Thu Feb 13 2025 16:49:26 GMT+0800","2025-02-14T23:59:09.999","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","All gymnasium equipment’s are not secured.","Miscellaneous","General Appearance","Behaviour Based","","","","","Gym equipments secured properly.","2025-03-14T23:59:09.999","","Completed","2025-02-27T23:59:09.999","No","No","No","Internal"]
[null,null,null,39358,87112,"55_Thu Feb 13 2025 16:56:07 GMT+0800","2025-02-14T23:59:09.999","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Rust marks on No.2 WBP to be cleaned and painted.","Cargo Mach.","","Equipment Related","","","","","No.2 WBP casing cleaned and painted.","2025-03-14T23:59:09.999","","Completed","2025-02-21T23:59:09.999","No","No","No","Internal"]
[null,null,null,39359,57949,"0_Sat Feb 15 2025 09:57:39 GMT+0800","2025-02-14T23:59:09.999","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","No.1 FWG solenoid valve connection is disconnected.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","No.1 FWG solenoid valve renewed","2025-03-14T23:59:09.999","","Completed","2025-01-29T23:59:09.999","No","No","No","Internal"]
[null,null,null,39343,92521,"55_Sun Feb 16 2025 17:28:59 GMT+0800","2025-02-16T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","Hose handling crane (STBD) change over block for man riding/cargo handling found malfunctioning.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","The change over block spool removed from place & found the locking pin broken. Same fabricated & fitted back. HHC - STBD tried out, found working satisfactory.","2025-05-16T23:59:09.999","","Completed","2025-02-16T23:59:09.999","No","No","No","Internal"]
[null,null,null,39349,52609,"55_Thu Feb 27 2025 04:36:54 GMT+0800","2025-02-17T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","MAIN DG NO 1 TURBOCHARGER WATER WASHING INLET LINE REMOVED AND FOUND COMPLETELY CHOKED.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","SAME FABRICATED WITH NEW.","2025-03-01T23:59:09.999","","Completed","2025-02-17T23:59:09.999","No","No","No","Internal"]
[null,null,null,39344,97230,"0_Thu Feb 27 2025 04:42:30 GMT+0800","2025-02-18T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","FORWARD HYDRAULIC PUMP NO 1 SPIDER COUPLING FOUND BROKEN.","Deck - Mooring Machinery","Mooring","Equipment Related","","","","","FORWARD HYDRAULIC PUMP NO 1 BROKEN SPIDER COUPLING REPLACED WITH NEW SPARE. PUMP TRIED OUT, FOUND WORKING SATISFACTORY.\n","2025-03-01T23:59:09.999","","Completed","2025-02-18T23:59:09.999","No","No","No","Internal"]
[null,null,null,39350,71729,"55_Fri Feb 21 2025 08:58:40 GMT+0800","2025-02-22T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","Wind speed Indicator's Display in CCR, reading is frozen.","Miscellaneous","Cargo / Ballast Systems","Equipment Related","","","","","Display Cable contact issue rectified.\nWind speed Indicator's display working satisfatorily.","2025-03-22T23:59:09.999","","Completed","2025-02-24T23:59:09.999","No","No","No","Internal"]
[null,null,null,39351,26689,"0_Thu Feb 27 2025 04:46:09 GMT+0800","2025-02-22T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","ER VENT FAN NO 3 CASING MESH SUPPORT FOUND BROKEN.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","","","","","ER VENT FAN NO 3 BROKEN CASING MESH SUPPORT FABRICATED NEW.\n","2025-03-01T23:59:09.999","","Completed","2025-02-23T23:59:09.999","No","No","No","Internal"]
[null,null,null,39353,78914,"0_Thu Feb 27 2025 04:48:11 GMT+0800","2025-02-22T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","GALLEY DRAIN LINE STORM VALVE ON E/R 2ND DECK FOUND LEAKING.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","GALLEY DRAIN LINE LEAKY STORM VALVE ON E/R 2ND DECK REPLACED WITH NEW SPARE","2025-03-01T23:59:09.999","","Completed","2025-02-23T23:59:09.999","No","No","No","Internal"]
[null,null,null,39354,71455,"55_Fri Feb 21 2025 08:51:31 GMT+0800","2025-02-22T23:59:09.999","Observation","Ship Staff","Ship Staff Insp.","Vapour manifold reducer's bottom plate of the hinge for the blank to be cropped and removed. Threaded stud on the presentation flange to be made permanent by welding the stud to the presentation flange as per Recommendations for Oil and Chemical Tanker Manifolds.","Cargo Mach.","Cargo / Ballast Systems","Behaviour Based","","","","","Vapour manifold reducers taken to E/Room Workshop and bottom plate of the hinge for the blank cropped and removed. Studs fixed permanent by welding.","2025-05-22T23:59:09.999","","Completed","2025-02-24T23:59:09.999","No","No","No","Internal"]
[null,null,null,39357,62693,"55_Sat Mar 01 2025 13:09:32 GMT+0800","2025-02-25T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","AUX BOILER #1 SWIRLER FOUND VIBRATING WHEN IN OPERTION.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","UPON REMOVAL OF THE # 1 AUX BOILER SWIRLER ASSEMBLY FOUND THE SUPPORTING LUGS WERE NOT TOUCHING THE CASING BODY AT THE BOTTOM & WAS HANGING LOOSE. THE LUGS FOUND TO BE WORN OUT & SAME WERE REBUILT BY WELDING & PUT BACK. # 1 BOILER TRIED OUT & FOUND WORKING SATISAFCTORY WITHOUT ANY VIBRATION.\n","2025-03-01T23:59:09.999","","Completed","2025-02-25T23:59:09.999","No","No","No","Internal"]
[null,null,null,39971,49146,"55_Thu Mar 20 2025 14:10:25 GMT+0800","2025-02-26T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","M/E TACHOMETER RPM DETECTOR 2/1 FOUND IN ALARM S/F CONDITION.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","",""," SENSOR REPLACED AND AIR GAP MEASURED AND KEPT 4MM AS PER MAKER MANUAL ALL RPM SENSORS CLEANED AND FUNCTION TESTED FOUND WORKING SATISFACTORY.","2025-05-26T23:59:09.999","","Completed","2025-03-15T23:59:09.999","No","No","No","Internal"]
[null,null,null,39325,63435,"0_Sat Mar 01 2025 13:15:27 GMT+0800","2025-03-01T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","HOSE HANDLING CRANE LIMIT SWITCH ASSEMBLY FOR PERSONNEL TRANSFER  FOUND FROZEN.","Deck - Machinery","Cargo / Ballast Systems","Equipment Related","","","","","Limit switches renewed & made operational.","2025-04-01T23:59:09.999","","Completed","2025-03-01T23:59:09.999","No","No","No","Internal","Noted. Job in progress. Pls expedite."]
[null,null,null,39973,93379,"55_Thu Mar 20 2025 13:09:06 GMT+0800","2025-03-02T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","AUX BOILER NO 1 FEED WATER CONTROLLER VALVE SIPART CONTROLLER FOUND MALFUNCTIONING.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","UPON INVESTIGATION FOUND THAT VALVE IS NOT OPENING AND CLOSING IN AUTO REPLACED PEIZO BLOCK AND REINITIALISED SIPART AND WAITED UNTIL AUTO CALIBRATION FINISHED. AFTER AUTO CALIBRATION FINISHED VALVE TESTED FOUND WORKING  IN GOOD ORDER. \n","2025-06-02T23:59:09.999","","Completed","2025-03-07T23:59:09.999","No","No","No","Internal"]
[null,null,null,39974,87239,"55_Thu Mar 20 2025 13:15:22 GMT+0800","2025-03-04T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","E.R. VENT FAN #2  VENT FLAP FOUND NOT CLOSING COMPLETELY","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","E.R. VENT FAN VENT FLAP PORTION WHICH WAS TOUCHING THE CASING GRINDED &  EASED UP. FLAP MADE TO CLOSE FULLY.\n","2025-06-04T23:59:09.999","","Completed","2025-03-04T23:59:09.999","No","No","No","Internal"]
[null,null,null,39965,65264,"55_Thu Mar 20 2025 13:16:59 GMT+0800","2025-03-06T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","FOAM PUMP MECHANICAL SEAL FOUND LEAKING. ","LSA / FFA","Emgcy. Systems","Equipment Related","","","","","MECHANICAL SEAL WAS RENEWED AND TRIED OUT AFTER RECEIVING CONCURRANCE FROM OFFICE.",null,"","Completed","2025-03-06T23:59:09.999","No","No","No","Internal"]
[null,null,null,39970,13495,"55_Thu Mar 20 2025 14:06:08 GMT+0800","2025-03-08T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","# 1 MAC CRANKSHAFT SURFACE FOUND WORN OUT IAT HP PISTON CONROD BIG END SEATING AREA","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","CRANKSHAFT RENEWED & COMPLETE O'HAUL CARRIED OUT.  HOWEVER WHILE TRYING OUT FOUND CRANKCASE PRESSURISED WHICH RESULTED IN PREVENTING THE LUBRICATION OF THE DRIVE END BEARING. HENCE BEARING GOT SEIZED. BOXED UP SPARE COMPRESOR FROM CHINA AND PUT IN TO SERVICE.","2025-06-07T23:59:09.999","","Completed","2025-03-18T23:59:09.999","No","No","No","Internal"]
[null,null,null,39961,26902,"55_Thu Mar 20 2025 14:37:46 GMT+0800","2025-03-12T23:59:09.999","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","# 1 Main cooling sea water pump mechnical seal cooling line found leaking of SW.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","","","","","The cooling water copper tube  renewed with new pipe.","2025-06-11T23:59:09.999","","Completed","2025-03-27T23:59:09.999","No","No","No","Internal","Pls renew pipe, as required."]
[null,null,null,39972,23235,"55_Thu Mar 20 2025 14:35:59 GMT+0800","2025-03-12T23:59:09.999","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","EGCS SW pumps discharge common manifold found leaking from hole.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Leak rectified by welding a doubler plate on the hole. ","2025-06-11T23:59:09.999","","Completed","2025-03-18T23:59:09.999","No","No","No","Internal"]
[null,null,null,39975,52361,"55_Thu Mar 20 2025 13:59:58 GMT+0800","2025-03-15T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","JCW FOUND COMING OUT FROM #1 MAIN DG UNIT #4, #5 & #6 CYL HEADS ","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","MAIN DG #1 UNIT #4, #5 & #6 REMOVED FROM PLACE AFTER AFTER SUSPECTION JCW LEAK. PRESSURE TESTED ALL 3 CYLINDER AND FOUND LEAK FROM UNIT #4 CYLINDER HEAD EXHAUST SIDE. SAME WAS REPLACED WITH NEW SPARE CYLINDER HEAD AND UNIT #5 AND #6 PUT BACK IN PLACE.","2025-06-15T23:59:09.999","","Completed","2025-03-15T23:59:09.999","No","No","No","Internal"]
[null,null,null,40142,67066,"0_Wed Mar 26 2025 06:10:01 GMT+0800","2025-03-21T23:59:09.999","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","VHF poster P70 not posted adjacent to VHF units on bridge\nas required by company QDMS","Miscellaneous","Communication","Human Error","","","","","VHF poster P70 posted adjacent to VHF units on bridge","2025-04-21T23:59:09.999","","Completed","2025-03-22T23:59:09.999","No","No","No","Internal"]
[null,null,null,40143,58947,"0_Wed Mar 26 2025 06:13:59 GMT+0800","2025-03-21T23:59:09.999","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Newly installed Starlink antenna to be marked on Monkey\nIsland and update Antenna plan/dwg accordingly","Miscellaneous","Communication","Human Error","","","","","Starlink antenna marked on Monkey\nIsland and updated Antenna plan/dwg accordingly.","2025-04-21T23:59:09.999","","Completed","2025-03-26T23:59:09.999","No","No","No","Internal"]
[null,null,null,40181,97224,"0_Sat Apr 12 2025 03:17:39 GMT+0800","2025-04-05T23:59:09.999","Defect","Ship Staff","Ship Staff Insp.","Both The gangway Shifting wires are overdue for replacement As per Company policy (2 Years)","Miscellaneous","ISM Related","Knowledge Based","","","","","New gangway shifting wires received. Will change the wires prior putting the gangways into use (prior reaching discharge port) and will test the gangway.\n","2025-07-05T23:59:09.999","SSUN240152","Completed","2025-04-05T23:59:09.999","No","No","No","Internal"]
[null,null,null,null,73890,"0_Wed Mar 26 2025 06:12:19 GMT+0800","2025-03-21T07:59:35","Non Conformity","Owner / Marine / Tech. Suptd.","Nav Audit / Verification","Old batteries stowed in Battery room. Same to re-locate to\nsuitable store and land ashore","Miscellaneous","Emgcy. Systems","Human Error","","","","","The stowed old batteries shifted from the battery room to garbage locker for landing at Singapore.","2025-05-01T07:59:35","","Completed","2025-04-04T07:59:35","No","No","No","Internal","Pls offland at next opportunity."]
[null,null,null,null,27036,"55_Thu Mar 20 2025 13:56:00 GMT+0800","2025-03-05T07:59:35","Defect","Ship Staff","Ship Staff Insp.","Elevator cage door found not properly closing. DOOR INVERTER and / or DOOR ENCODER is malfunctioning.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","Service Technician attended to the problem at Puerto Armuelles , door inverter PCB and configured. The elevator tried out and found to be working satisfactory. The problem resolved.","2025-06-04T07:59:35","","Completed","2025-04-13T07:59:35","No","No","No","Internal","Spares will be connected in Panama."]
[null,null,null,null,14989,"55_Sun Feb 16 2025 16:38:53 GMT+0800","2025-02-16T07:59:35","Defect","Ship Staff","Ship Staff Insp.","Main D/G spare cylinder heads(2 no's) found damaged on exhaust valve seat housing","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","2 pcs new spare cylinder head received at ECO PAL and kept as spare.","2025-05-16T07:59:35","RO - SSUN250060","Completed","2025-03-20T07:59:35","No","No","No","Internal","Spare cylinder heads will be connected in PAL."]
[null,null,null,null,25097,"55_Mon Jan 06 2025 10:10:00 GMT+0800","2025-01-11T07:59:35","Critical Equipment","Ship Staff","Ship Staff Insp.","EMERGENCY SWITCH BOARD CONTROL CIRCUIT RELAYS AND TIMERS TO BE RENEWED","Elect. Mach. & Equip.","Emgcy. Systems","Equipment Related","","","","","All timers and relays replaced by new spares.","2025-05-11T07:59:35","","Completed","2025-01-20T07:59:35","No","No","No","Internal","Pls expedite."]
[null,null,null,null,97624,"55_Mon Feb 10 2025 08:39:27 GMT+0800","2025-02-04T07:59:35","Defect","Ship Staff","Ship Staff Insp.","Aux D/G T/C LO found leaking on the turbine side through radial plain bearing","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","The cartridge renewed with the one received from DHT Amazon , tried out and working satisfactory.","2025-05-02T07:59:35","","Completed","2025-03-23T07:59:35","No","No","No","Internal","Spare cartridge from EX-AMAZON supplied to vsl."]
[null,null,null,null,22772,"55_Sat Feb 15 2025 09:38:49 GMT+0800","2025-02-14T07:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Exhaust gas leak from WHRS manhole cover.","E/R - Pipes/ valves & fittings","","","","","","","The gaskets of all the manhole doors , 10 in nos. renewed with ceramic fibre tapes material","2025-05-13T07:59:35","","Completed","2025-04-10T07:59:35","No","No","No","Internal","This is critical, as the exhaust gas leaking from the manhole. Pls inspect at next suitable opportunity."]
[null,null,null,null,17973,"55_Sat Mar 01 2025 10:53:38 GMT+0800","2025-03-01T07:59:35","Critical Equipment","Ship Staff","Ship Staff Insp.","Both Lifeboats top FRP hatch covers found frozen.","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","Both Lifeboat Hatchcovers freed","2025-04-01T07:59:35","","Completed","2025-04-21T07:59:35","No","No","No","Internal","Noted. Pls expedite."]
[null,null,null,null,99690,"0_Wed Mar 26 2025 07:01:27 GMT+0800","2025-03-21T07:59:35","Observation","Owner / Marine / Tech. Suptd.","Mooring Audit","Mooring winches to be marked with hydraulic test pressure\napplied for brake setting on each winch","Deck - Mooring Machinery","Mooring","Equipment Related","","","","","Mooring winches stencilled with hydraulic test pressure\napplied for brake setting.","2025-05-21T07:59:35","","Completed","2025-04-15T07:59:35","No","No","No","Internal","Pls carry out the job and update."]
[null,null,null,null,91369,"55_Wed Mar 26 2025 07:07:38 GMT+0800","2025-03-21T07:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Fire control station - remove stock of spare fire\nextinguisher charges and re-locate in suitable store","LSA / FFA","Safety / LSA / FFA","Human Error","","","","","Spare fire extinguisher charges  relocated .","2025-04-21T07:59:35","","Completed","2025-05-01T07:59:35","No","No","No","Internal","Pls do as required."]
[null,null,null,null,22179,"55_Thu Feb 13 2025 16:47:50 GMT+0800","2025-02-14T07:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Dry prov. room, Ac room, Accom entrance door rainwater protection plate is corroded.","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","Equipment Related","","","","","W/T doors eye brows needs temporary repairs.\nPermanent repairs to be carried out during next DD.","2025-05-14T07:59:35","","Completed","2025-04-20T07:59:35","No","No","No","Internal","Pls plan during next ballast passage."]
[null,null,null,null,83487,"55_Thu Feb 13 2025 16:53:48 GMT+0800","2025-02-14T07:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Few checker plates for ramps on deck are rusted","Deck - Pipe / Fittings","General Appearance","External Factors","","","","","Job completed","2025-04-01T07:59:35","","Completed","2025-03-26T07:59:35","No","No","No","Internal","Pls carry out maintenance."]
[null,null,null,null,77772,"0_Wed Mar 26 2025 06:59:41 GMT+0800","2025-03-21T07:59:35","Observation","Owner / Marine / Tech. Suptd.","Mooring Audit","Total 23 Tonsberg mooring shackles not compliant with\nMEG4 MBL requirement","Deck - Mooring Machinery","Mooring","Equipment Related","","","","","To renew with Tonsberg mooring shackles which meets MEG4 standards.","2025-06-21T07:59:35","","Completed","2025-02-06T07:59:35","No","No","No","Internal","Pls create RO as required."]
[null,null,null,null,98442,"55_Wed Mar 26 2025 06:08:05 GMT+0800","2025-03-21T07:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Bio-Fouling file does not contain any record for cleaning of\nBallast pump and BWTS filters. Same recommended to be\nmaintained","Documentation","Cert. & Docu.","Human Error","","","",""," Records for cleaning of ballast pumps and BWTS filters filed in the Bio fouling file.","2025-06-21T07:59:35","","Completed","2025-04-25T07:59:35","No","No","No","Internal","Pls make relevant entries as required."]
[null,null,null,null,26726,"0_Sat Feb 15 2025 09:47:47 GMT+0800","2025-02-14T07:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Main engine spare cylinder cover to be assembled with exhaust valve, cylinder jacket and other accessories.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Spare Exhaust valve overhauled and fitted on the Main Engine Spare cylinder cover.","2025-04-26T07:59:35","","Completed","2025-05-01T07:59:35","No","No","No","Internal","Pls expedite."]
[null,null,null,null,33455,"55_Sun Jun 15 2025 15:47:18 GMT+0800","2025-05-29T08:00:00","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","All holes on the fire door and bulkheads to be closed with flat head screws","Accommodation","General Appearance","Inappropriate Procedure","","","","","Job completed.","2025-06-13T08:00:00","","Completed","2025-06-15T08:00:00","No","No","No","Internal"]
[null,null,null,null,99045,"0_Sat Apr 12 2025 03:09:38 GMT+0800","2025-04-04T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Fwd windlass STBD side inboard & Outboard mooring winch is having an abnormal noise and wobbling while operation.","Deck - Mooring Machinery","Mooring","Equipment Related","","","","","Windlaas is operational, we have used this windlass / Anchor during last port of call Fujairah in July 2024 for anchoring. Also we have used stbd windlass & winch during port operations in Europe. During this operation noted inboard & outboard winch is operational with slight Wobbling though it does not effects winch operation. By greasing prior operation noted that wobbling intensity reduces. please not below comments in REFMAN made during last repairs by ship staff. REFMAN COMMENTS: 10-MAR-2023 : By user Spare parts can be ordered just before the next drydock which is planned feb 2027. Vessel have replaced the sleeve bearing os split drum but noticed shaft to be worn off more than the limits. As of now no wobbling but wobbling can take place in future after certain period of use. Refman Job raised in 2023\"","2025-07-04T08:00:00","Staffa motor changed on  06-05-2025. now working satisfactory  ","Completed","2025-05-06T08:00:00","No","No","No","Internal"]
[null,null,null,null,98815,"55_Sat Apr 12 2025 03:42:38 GMT+0800","2025-04-02T08:00:00","Defect","Ship Staff","Ship Staff Insp.","During inspection of Pumproom Neil Robertson stretcher securing belts found in damaged condition because of aging of belts","Miscellaneous","","External Factors","","","","","Neil Robertson stretcher replaced by new one.","2025-07-01T08:00:00","SSUN250099","Completed","2025-05-31T08:00:00","No","No","No","Internal"]
[null,null,null,null,65730,"55_Wed Mar 26 2025 06:57:39 GMT+0800","2025-03-21T08:00:00","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Stbd windlass staffa motor is noisy in operation. Internal\noil leakage is suspected. Same to verify and repair.","Deck - Mooring Machinery","Mooring","Equipment Related","","","","","Internal leakage test has been carried out on Stbd. windlass staffa motor and the leakage qty. is observed to be more(Approx.4 – 5 ltrs) than the recommended(3 ltrs). Stbd. windlass was last used in Basrah on 25 Jan 2025 when the noise was observed, after that windlass has not been used and will not be used for anchoring purpose. The operation of mooring winch is satisfactory and same was last used at Echo PAL without any issues. Vessel has spare staffa motor and suggest to renew the Stbd. windlass staffa motor after discharging operation in China enroute to Singapore. If any problems arise, additional shore assistance can be arranged in Singapore during the vessel's call for bunkering/storing.\nLeakage test was also carried out on port windlass staffa motor and no internal leakage observed.","2025-06-21T08:00:00","Staffa motor changed on  06-05-2025. now working satisfactory  ","Completed","2025-05-06T08:00:00","No","No","No","Internal","Pls remove defect, if rectified."]
[null,null,null,null,26548,"55_Fri Feb 21 2025 08:32:24 GMT+0800","2025-02-22T08:00:00","Defect","Ship Staff","Ship Staff Insp.","1. Stbd windlass auto speed changeover lever is frozen.\n2. Leak observed on Stbd. windlass operating lever.","Deck - Mooring Machinery","Mooring","Equipment Related","","","","","1. The auto speed changeover block renewed. \n2.  Stbd. windlass operating lever o-ring renewed.","2025-05-22T08:00:00","","Completed","2025-05-06T08:00:00","No","No","No","Internal","Pls take up this job on priority."]
[null,null,null,null,94449,"55_Fri Sep 06 2024 21:01:14 GMT+0800","2025-01-15T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Hydro blaster is in operational","Deck - Machinery","General Appearance","Equipment Related","","","","","spare received and renewed as required, Now Hydro blaster working satisfactory.\n","2025-04-16T08:00:00","SSUN250066","Completed","2025-05-31T08:00:00","No","No","No","Internal","Pls check and revert."]
[null,null,null,null,89484,"55_Wed Mar 19 2025 21:06:23 GMT+0800","2025-03-16T08:00:00","Defect","Ship Staff","Ship Staff Insp.","IGS scrubber SW common manifold inlet to the nozzle sections are having pin holes.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Renewed ","2025-06-16T08:00:00","","Completed","2025-03-25T08:00:00","No","No","No","Internal","pls carry out the job at next suitable opportunity."]
[null,null,null,null,68045,"55_Sun Jun 15 2025 15:36:52 GMT+0800","2025-05-29T08:00:00","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Deck Seal flow control valve gland is leaking","Inert Gas","Cargo / Ballast Systems","Equipment Related","","","","","Gland Tightened and the leak rectified.","2025-06-29T08:00:00","","Completed","2025-06-17T08:00:00","No","No","No","Internal"]
[null,null,null,null,26743,"0_Sat Apr 12 2025 03:02:37 GMT+0800","2025-04-03T08:00:00","Defect","Ship Staff","Ship Staff Insp.","No.2 Ballast BWTS Filter Inlet Line found holed","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","","","","","Cold work carried out, leak is on filter casing flange and filter can't be removed. Need to carry out hotwork in place, job Raised in Refman for next DD.\n","2025-07-03T08:00:00","","Completed",null,"No","No","No","Internal"]
[null,null,null,null,24669,"0_Wed Mar 26 2025 06:54:04 GMT+0800","2025-03-21T08:00:00","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Ballast tanks indicate CO gas after deballasting. Suspect\nthis is H2 gas carried over from BWTS. Same to be\ninvestigated and rectify.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","Vessel opened up Gas separator of BWTS Electrolyzer unit. and verified the operation of the auto vent valve. No scaling or deposition was found inside the gas separator. The auto vent valve was opened and checked and it is functioning correctly. No damage was observed to the float arrangement. Investigation is completed.\nThis is because of cross sensitivity  of sensor.","2025-06-21T08:00:00","","Completed",null,"No","No","No","Internal","Pls revert after completion of investigation."]
[null,null,null,null,45810,"55_Sat Apr 12 2025 02:38:24 GMT+0800","2025-03-29T08:00:00","Defect","Ship Staff","Ship Staff Insp.","FPK Ballast tank & 5P WBT Remote level gauge in CCR is not working\n\n","Miscellaneous","Cargo / Ballast Systems","Equipment Related","","","","","RO  SSUN240130 received, PCB replaced for FPK tank transmitter, but the trouble still exists. Trouble shooting is in progress.\nDuplication of defect in DDRL.","2025-06-29T08:00:00","RO  SSUN240130","Completed",null,"No","No","No","Internal"]
[null,null,null,null,93827,"0_Sun Dec 15 2024 15:56:48 GMT+0800","2024-11-21T08:00:00","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Fittings, railing and vertical ladder on light masts on deck need to derusted and maintenance to be carried out.","Deck - Pipe / Fittings","General Appearance","Equipment Related","","","","","Fittings, railing and vertical ladder on light masts on deck need derusted and maintenance to be carried out.","2025-06-06T08:00:00","","Completed","2025-07-07T08:00:00","No","No","No","Internal","Pls expedite."]
[null,null,null,null,22825,"0_Sun Jun 15 2025 15:41:14 GMT+0800","2025-05-29T08:00:00","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Main Engine rail area to clean","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Main Engine rail area cleaned.","2025-07-29T08:00:00","","Completed","2025-07-16T08:00:00","No","No","No","Internal"]
[null,null,null,null,48054,"0_Sun Jun 15 2025 15:38:38 GMT+0800","2025-05-29T08:00:00","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","LP Drum Port Side gauge glass is leaking","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","The L P Drum Port side gauge glass overhauled, the leak rectified.","2025-07-29T08:00:00","","Completed","2025-07-14T08:00:00","No","No","No","Internal"]
[null,null,null,null,79194,"55_Sun Feb 16 2025 17:36:46 GMT+0800","2025-02-04T08:00:00","Defect","Ship Staff","Ship Staff Insp.","# 2 FWG Ejector pump found leaking from the mech seal.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","","","","","#2FWG Ejector Pump Overhauled, The shaft, mechanical seal, cover, impeller nut and the line bearing cover renewed with new spare .","2025-05-04T08:00:00","RO -  SSUN250065","Completed","2025-07-23T08:00:00","No","No","No","Internal","PO is approved. Spares will be connected at next suitable port."]
[null,null,null,null,55608,"0_Sun Jun 15 2025 15:39:48 GMT+0800","2025-05-29T08:00:00","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","LP Drum feed water inlet control valve air regulator is leaking","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","","","","","The leak on the air regulator rectified.","2025-07-29T08:00:00","","Completed","2025-07-18T08:00:00","No","No","No","Internal"]
[null,null,null,null,99790,"0_Sun Jun 15 2025 15:42:27 GMT+0800","2025-05-29T08:00:00","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Main Engine both turbochargers manometer to clean","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","","","","","The Manometers cleaned","2025-07-29T08:00:00","","Completed","2025-06-21T08:00:00","No","No","No","Internal"]
[null,null,null,null,80631,"55_Thu Mar 20 2025 14:31:50 GMT+0800","2025-03-12T08:00:00","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","# 1 FWG is not operational","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","The Ejector Pump overhauled and the distillate pump renewed with new spare. ","2025-06-11T08:00:00","","Completed","2025-07-24T08:00:00","No","No","No","Internal","Pls carry out troubleshooting and revert."]
[null,null,null,null,20819,"55_Tue Apr 16 2024 19:03:47 GMT+0800","2025-01-04T08:00:00","Observation","Ship Staff","Ship Staff Insp.","Pin hole on the icu return pipeline(non pressure side) going back to the sump.","E/R - Main Engine,E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Industry Issue,Equipment Related","10.29","Medium","","","Leak has been rectified.","2025-07-01T08:00:00","SSUN 240110","Completed","2025-05-29T08:00:00","No","No","No","Internal","spares supplied during last port call, pls. check and try to renew at suitable opportunity."]
[null,null,null,null,73980,"55_Wed Jan 15 2025 23:22:10 GMT+0800","2025-01-17T08:00:00","Defect","Ship Staff","Ship Staff Insp.","CO2 room O2 sensor found malfunctioning","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","The sensor calibrated and the fault rectified.","2025-04-17T08:00:00","SSUN255014","Completed","2025-04-16T08:00:00","No","No","No","Internal","Pls liaise with autoelec dept."]
[null,null,null,null,45869,"55_Thu Jun 12 2025 13:56:08 GMT+0800","2025-06-02T08:00:00","Defect","Ship Staff","Ship Staff Insp.","1P Ballast tank Remote level gauge in CCR is not working","Miscellaneous","Cargo / Ballast Systems","Equipment Related","","","","","Level Sensor renewed with new spare and calibrated. Found working satisfactory.","2025-09-30T08:00:00","","Completed","2025-08-12T08:00:00","No","No","No","Internal"]
[null,null,null,null,40980,"0_Sat Jun 01 2024 16:41:36 GMT+0800","2024-11-17T08:00:00","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","IBC tanks kept on top of Emergency generator room to be cleaned and covered in sunshade area to use for future maintenance.","Miscellaneous","General Appearance","External Factors","","","","","Job completed","2025-06-16T08:00:00","","Completed","2025-08-03T08:00:00","No","No","No","Internal","Noted ."]
[null,null,null,null,80282,"55_Sat Apr 12 2025 02:26:01 GMT+0800","2025-03-28T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Drain PIpe on Main IG line connecting to IG to Ballast Line spool piece on Main Deck found wasted.","Inert Gas,Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","","","","","Cold work carried out , the pipe is too big to remove by the ship staff and take it to the workshop need shore assistance for the said job. JOB HAS BEEN DEFERRED TI DRY DOCK.","2025-07-28T08:00:00","","Completed","2025-07-28T08:00:00","No","No","No","Internal"]
[null,null,null,null,79385,"55_Sat Apr 12 2025 02:29:07 GMT+0800","2025-03-28T08:00:00","Defect","Ship Staff","Ship Staff Insp.","EGCS SYSTEM, JET UNIT VALVE XV_1_2070A, DISTANCE PIECE BETWEEN JET UNIT AND VALVE HAD DEVELOPED A HOLE IN THE PIPE WELDING SEAM, SINCE FUEL WAS CHANGED TO LSMGO AND EGCS WAS STOPPED, SAME PIPE WAS TAKEN OUT REPAIRED AND PUT BACK, ","E/R - Aux. Engine,E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.11","Medium","","","SINCE FUEL WAS CHANGED TO LSMGO AND EGCS WAS STOPPED, SAME PIPE WAS TAKEN OUT REPAIRED AND PUT BACK,  OVER THE PERIOD SAME PIPE NEED TO BE REPLACE WITH NEW ONE. PRESENTLY NO LEAKS.\n","2025-06-28T08:00:00","","Completed","2025-06-28T08:00:00","No","No","No","Internal"]
[null,null,null,null,16307,"55_Sat Apr 12 2025 00:11:56 GMT+0800","2024-06-13T08:00:00","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Emergency generator room conduit access was noted holed with the cover missing ","Elect. Mach. & Equip.","General Appearance","Equipment Related","","","","","Need to rectify by welding , at the moment it has been rectified by soft patch and the end cover fixed. JOB DEFERRED TO DRY DOCK","2025-06-01T08:00:00","","Completed",null,"No","No","No","Internal","Plan to fabricate and repair the cover."]
[null,null,null,null,32907,"55_Thu Feb 13 2025 17:03:28 GMT+0800","2025-02-13T08:00:00","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","AHU room water leak observed on the common air duct and lagging is in poor condition.","Elect. Mach. & Equip.","","Equipment Related","","","","","To identify the source of leak and to rectify. To renew the lagging as required. JOB DEFERRED TO DRY DOCK.","2025-05-14T08:00:00","","Completed","2025-05-14T08:00:00","No","No","No","Internal","Pls inspect and revert with condition."]
[null,null,null,null,31171,"55_Wed Aug 20 2025 22:34:51 GMT+0800","2025-02-13T08:00:00","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Sea water leaks on the FWG to be rectified","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","FWG leaks rectified and system made operational. system tried out and working satisfactory.","2025-05-13T08:00:00","","Completed","2025-05-12T08:00:00","No","No","No","Internal","Identify the leaks and rectify"]
[null,null,null,39977,null,"55_Fri Mar 21 2025 02:15:17 GMT+0000","2025-07-20T08:00:00","Observation","Ship Staff","Ship Staff Insp.","Steam ballast pump when used for ballasting parallel to electric ballast pump BWTS system trips off. Vessel noticed this during last port while ballasting operation. As per records steam ballast pump on deballast works perfectly during ballasting operation trips BWTS system.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","Both the Ballast Pumps are running satisfactorily individually. ","2025-10-20T08:00:00","","Completed","2025-08-27T08:00:00","No","No","No","Internal","Pls carry out troubleshooting and revert with findings."]
[null,null,null,null,41486,"0_Sat Apr 12 2025 03:20:11 GMT+0800","2025-08-15T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Fan failure fault on Conning display unit at Wheel house","Elect. Mach. & Equip.","Navigation","Equipment Related","","","","","Presently the system is working satisfactorily without any alarms","2025-11-15T08:00:00","","Completed","2025-08-27T08:00:00","No","No","No","Internal",""]
[null,null,null,null,41038,"55_Thu Feb 13 2025 17:00:43 GMT+0800","2025-02-13T08:00:00","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Both pantry’s hot water boiler is not working.","Miscellaneous","Safety / LSA / FFA","Equipment Related","","","","","Each Pantry has been supplied with individual hot water dispenser.","2025-05-13T08:00:00","","Completed","2025-05-10T08:00:00","No","No","No","Internal","PO is still under processing."]

{"sheet":"Calc","index":2,"n_rows":28,"n_cols":12,"rows_kept":28,"cut":false,"hidden":true,"merged":[]}
["Def_type","Def_cause","Equipments","VIQrefno","Observer_code"]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,"Dim itemSele As Long"]
[null,null,null,null,null,null,null,null,null,null,null,"   dim startRow as integer"]
[null,null,null,null,null,null,null,null,null,null,null,"   startRow=1"]
[null,null,null,null,null,null,null,null,null,null,null,"        For itemSele = 0 To ListBox1.ListCount - 1"]
[null,null,null,null,null,null,null,null,null,null,null,"        If ListBox1.Selected(itemSele) = True Then"]
[null,null,null,null,null,null,null,null,null,null,null,"        Worksheets(\"WorksheetName\").Range(\"A\" & startRow).Value = ListBox1.List(itemSele)"]
[null,null,null,null,null,null,null,null,null,null,null,"        startRow = startRow + 1"]
[null,null,null,null,null,null,null,null,null,null,null,"        End If"]
[null,null,null,null,null,null,null,null,null,null,null,"        Next"]
[null,null,null,null,null,null,null,null,null,null,null,"Dim LastRowA As String"]
[null,null,null,null,null,null,null,null,null,null,null,"        Dim itemSele As Long"]
[null,null,null,null,null,null,null,null,null,null,null,"       Dim startRow as integer"]
[null,null,null,null,null,null,null,null,null,null,null,"        LastRowA = ActiveSheet.Cells(Rows.count, \"A\").End(xlUp).row"]
[null,null,null,null,null,null,null,null,null,null,null,"        startQue = 0"]
[null,null,null,null,null,null,null,null,null,null,null,"        For itemSele = 0 To ListBox1.ListCount - 1"]
[null,null,null,null,null,null,null,null,null,null,null,"        For startRow = 1 To LastRowA"]
[null,null,null,null,null,null,null,null,null,null,null,"        If Worksheets(\"WorksheetName\").Range(\"A\" & startRow).Value = ListBox1.List(itemSele) Then"]
[null,null,null,null,null,null,null,null,null,null,null,"        ListBox1.Selected(itemSele) = True"]
[null,null,null,null,null,null,null,null,null,null,null,"        Exit For"]
[null,null,null,null,null,null,null,null,null,null,null,"        End If"]
[null,null,null,null,null,null,null,null,null,null,null,"        Next j"]
[null,null,null,null,null,null,null,null,null,null,null,"        Next"]
[null,null,null,null,null,null,null,null,null,null,null,"        End If"]

{"sheet":"Areaofobs","index":3,"n_rows":17,"n_cols":2,"rows_kept":17,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Cargo / Ballast Systems",11]
["Cert. & Docu.",2]
["Communication",6]
["Crew Management",3]
["Emgcy. Systems",13]
["Eng. / Strg. Comp.",14]
["General Appearance",15]
["Ice Opns.",17]
["ISM Related",7]
["ISPS Related",10]
["MARPOL Related",9]
["MLC Related",4]
["Mooring",12]
["Navigation",5]
["Safety / LSA / FFA",8]
["Structural Condn. / WT integrity ",16]

{"sheet":"Vessel_type","index":4,"n_rows":1,"n_cols":2,"rows_kept":1,"cut":false,"hidden":true,"merged":[]}
["Vessel_type","ID"]

{"sheet":"Deficiency_type","index":5,"n_rows":8,"n_cols":3,"rows_kept":8,"cut":false,"hidden":true,"merged":[]}
["TITLE","Type of deficiency_description","ID"]
["Breakdown",null,6]
["Critical Equipment",null,4]
["Defect",null,1]
["Guarantee Claim",null,8]
["Non Conformity",null,2]
["Observation",null,3]
["Other",null,7]

{"sheet":"VIQrefno","index":6,"n_rows":427,"n_cols":3,"rows_kept":427,"cut":false,"hidden":true,"merged":[]}
["VIQ_ref_no","Risk Value of observation","ID"]
["1.1","Low",8243]
["1.10","Low",8252]
["1.11","Low",8253]
["1.12","Low",8254]
["1.13","Low",8255]
["1.14","Low",8256]
["1.15","Low",8257]
["1.16","Low",8259]
["1.17","Low",8260]
["1.18","Low",8261]
["1.19","Low",8262]
["1.2","Low",8244]
["1.20","Low",8263]
["1.21","Low",8265]
["1.22","Low",8266]
["1.23","Low",8267]
["1.24","Low",8268]
["1.25","Low",8269]
["1.26","Low",8270]
["1.3","Low",8245]
["1.4","Low",8246]
["1.5","Low",8247]
["1.6","Low",8248]
["1.7","Low",8249]
["1.8","Low",8250]
["1.9","Low",8251]
["1.99","High",11258]
["10.1","Medium",8461]
["10.10","High",8470]
["10.11","Medium",8471]
["10.12","Very High",8472]
["10.13","Very High",8473]
["10.14","Medium",8474]
["10.15","Low",8475]
["10.16","Very High",8476]
["10.17","Very High",8477]
["10.18","High",8478]
["10.19","Very High",8479]
["10.2","Low",8462]
["10.20","High",8480]
["10.21","Medium",8481]
["10.22","Low",8482]
["10.23","Medium",8483]
["10.24","Low",8484]
["10.25","Very High",8485]
["10.26","High",8486]
["10.27","Medium",8487]
["10.28","Low",8488]
["10.29","Medium",8489]
["10.3","Medium",8463]
["10.30","High",8490]
["10.31","Very High",8491]
["10.32","Very High",8492]
["10.33","High",8493]
["10.34","High",8494]
["10.35","Very High",8495]
["10.36","Very High",8496]
["10.37","Medium",8497]
["10.38","Medium",8498]
["10.39","High",8499]
["10.4","High",8464]
["10.40","Medium",8500]
["10.41","Medium",8501]
["10.42","Medium",8502]
["10.43","Medium",8503]
["10.44","Medium",8504]
["10.45","Very High",8505]
["10.46","High",8506]
["10.47","Medium",8507]
["10.48","High",8508]
["10.49","Medium",8509]
["10.5","Low",8465]
["10.50","High",8510]
["10.51","Low",8511]
["10.52","Medium",8512]
["10.53","Medium",8513]
["10.54","High",8514]
["10.55","Low",8515]
["10.6","Very High",8466]
["10.7","Medium",8467]
["10.8","Medium",8468]
["10.9","Medium",8469]
["10.99","High",8516]
["11.1","High",8420]
["11.10","Medium",8429]
["11.11","Very High",8430]
["11.12","Low",8431]
["11.13","Low",8432]
["11.14","Medium",8433]
["11.15","Low",8434]
["11.16","Low",8435]
["11.17","Low",8436]
["11.2","Medium",8421]
["11.3","Medium",8422]
["11.4","Very High",8423]
["11.5","Medium",8424]
["11.6","Medium",8425]
["11.7","High",8426]
["11.8","Low",8427]
["11.9","Low",8428]
["11.99","High",8437]
["12.1","High",8438]
["12.10","High",8448]
["12.11","High",8449]
["12.12","High",8450]
["12.13","High",8451]
["12.14","High",8452]
["12.15","High",8453]
["12.16","High",8454]
["12.17","High",8455]
["12.18","High",8456]
["12.19","High",8457]
["12.2","High",8439]
["12.20","High",8458]
["12.21","High",8459]
["12.3","High",8441]
["12.4","High",8442]
["12.5","High",8443]
["12.6","High",8444]
["12.7","High",8445]
["12.8","High",8446]
["12.9","High",8447]
["12.99","High",8460]
["2.1","Very High",8296]
["2.1.9","Very High",11259]
["2.10","Medium",8304]
["2.11","Medium",8305]
["2.12","Low",8306]
["2.13","Low",8307]
["2.14","Low",8308]
["2.15","Low",8309]
["2.16","Medium",8310]
["2.2","Medium",8297]
["2.3","High",8295]
["2.4","Medium",8298]
["2.5","Medium",8299]
["2.6","Low",8300]
["2.7","High",8301]
["2.8","High",8302]
["2.9","Medium",8303]
["2.99","High",8311]
["3.1","High",8312]
["3.2","Very High",8313]
["3.3","High",8314]
["3.4","Low",8294]
["3.5","Medium",8315]
["3.6","High",8316]
["3.7","Very High",8317]
["3.8","Very High",8318]
["3.99","High",8319]
["4.1","High",8320]
["4.10","High",8329]
["4.11","Medium",8330]
["4.12","Very High",8331]
["4.13","Very High",8332]
["4.14","Very High",8333]
["4.15","Very High",8334]
["4.16","Very High",8335]
["4.17","Very High",8336]
["4.18","Very High",8337]
["4.19","Low",8338]
["4.2","Medium",8321]
["4.20","Very High",8339]
["4.21","High",8340]
["4.22","Low",8341]
["4.23","High",8342]
["4.24","High",8343]
["4.25","Low",8344]
["4.26","Low",8345]
["4.27","High",8346]
["4.3","Medium",8322]
["4.4","High",8323]
["4.5","Very High",8324]
["4.6","Medium",8325]
["4.7","High",8326]
["4.8","Medium",8327]
["4.9","Medium",8328]
["4.99","High",8347]
["5.1","Very High",8517]
["5.10","High",8526]
["5.11","Low",8527]
["5.12","Medium",8528]
["5.13","High",8529]
["5.14","Very High",8530]
["5.15","Medium",8531]
["5.16","Very High",8532]
["5.17","Very High",8533]
["5.18","High",8534]
["5.19","Medium",8535]
["5.2","Very High",8518]
["5.20","Medium",8536]
["5.21","Medium",8537]
["5.22","High",8539]
["5.23","Very High",8540]
["5.24","Very High",8541]
["5.25","Medium",8542]
["5.26","Medium",8543]
["5.27","Medium",8544]
["5.28","Very High",8545]
["5.29","High",8546]
["5.3","Low",8519]
["5.30","High",8547]
["5.31","High",8548]
["5.32","High",8549]
["5.33","High",8550]
["5.34","Low",8551]
["5.35","Medium",8552]
["5.36","Low",8553]
["5.37","Low",8554]
["5.38","High",8555]
["5.39","Very High",8556]
["5.4","High",8520]
["5.40","Very High",8557]
["5.41","Very High",8558]
["5.42","Medium",8559]
["5.43","High",8560]
["5.44","High",8561]
["5.45","Medium",8564]
["5.46","Medium",8565]
["5.47","Medium",8566]
["5.48","Medium",8567]
["5.5","Low",8521]
["5.6","Low",8522]
["5.7","Medium",8523]
["5.8","Medium",8524]
["5.9","Very High",8525]
["5.99","High",8568]
["6.1","Medium",8348]
["6.10","Low",8357]
["6.11","High",8358]
["6.12","Medium",8359]
["6.13","Low",8360]
["6.14","High",8361]
["6.15","High",8362]
["6.16","Very High",8363]
["6.17","Very High",8364]
["6.18","Medium",8365]
["6.19","Low",8366]
["6.2","High",8349]
["6.20","Medium",8367]
["6.21","High",8368]
["6.22","Medium",8369]
["6.3","Low",8350]
["6.4","High",8351]
["6.5","Medium",8352]
["6.6","Medium",8353]
["6.7","High",8354]
["6.8","High",8355]
["6.9","Low",8356]
["6.99","High",8370]
["7.1","High",8371]
["7.10","High",8380]
["7.11","High",8381]
["7.12","High",8382]
["7.13","Medium",8383]
["7.14","Medium",8384]
["7.15","High",8385]
["7.16","High",8386]
["7.17","High",8387]
["7.2","High",8372]
["7.3","Low",8373]
["7.4","Low",8374]
["7.5","Low",8375]
["7.6","Medium",8376]
["7.7","Low",8377]
["7.8","High",8378]
["7.9","High",8379]
["7.99","High",8388]
["8.1","Very High",8569]
["8.10","Very High",8578]
["8.100","Low",11227]
["8.101","Medium",11228]
["8.102","Low",11229]
["8.103","Low",11230]
["8.104","Low",11231]
["8.105","Medium",11232]
["8.106","Medium",11233]
["8.107","Low",11234]
["8.108","High",11235]
["8.109","Very High",11236]
["8.11","Medium",8579]
["8.110","High",11237]
["8.111","Medium",11238]
["8.112","High",11239]
["8.113","Medium",11240]
["8.114","Low",11241]
["8.115","High",11242]
["8.116","Medium",11243]
["8.117","Medium",11244]
["8.118","Medium",11245]
["8.119","High",11246]
["8.12","Medium",8580]
["8.120","High",11247]
["8.121","Medium",11248]
["8.122","High",11249]
["8.123","High",11250]
["8.124","Low",11251]
["8.125","High",11252]
["8.126","Medium",11253]
["8.127","Medium",11254]
["8.13","Medium",8581]
["8.14","Very High",8582]
["8.15","High",8583]
["8.16","Very High",8584]
["8.17","Low",8585]
["8.18","High",8586]
["8.19","High",8587]
["8.199","High",11255]
["8.2","Medium",8570]
["8.20","Medium",8588]
["8.21","High",8589]
["8.22","Very High",8590]
["8.23","Medium",8591]
["8.24","Medium",8592]
["8.25","Very High",8593]
["8.26","High",8594]
["8.27","Medium",8595]
["8.28","Medium",8596]
["8.29","High",8598]
["8.3","Very High",8571]
["8.30","High",8599]
["8.31","High",8600]
["8.32","Low",8601]
["8.33","Medium",8602]
["8.34","High",8603]
["8.35","Medium",8604]
["8.36","Medium",8605]
["8.37","High",8607]
["8.38","Medium",8608]
["8.39","Medium",8609]
["8.4","Medium",8572]
["8.40","High",8610]
["8.41","Medium",8611]
["8.42","Medium",8612]
["8.43","Very High",8613]
["8.44","High",8615]
["8.45","High",8616]
["8.46","Very High",8617]
["8.47","Very High",8618]
["8.48","Medium",8619]
["8.49","High",8620]
["8.5","Very High",8573]
["8.50","Medium",8621]
["8.51","Low",8622]
["8.52","Low",8623]
["8.53","Low",8624]
["8.54","High",8625]
["8.55","Low",11182]
["8.56","Medium",11183]
["8.57","Medium",11184]
["8.58","High",11185]
["8.59","High",11186]
["8.6","Medium",8574]
["8.60","High",11187]
["8.61","Medium",11188]
["8.62","Very High",11189]
["8.63","High",11190]
["8.64","Medium",11191]
["8.65","Low",11192]
["8.66","High",11193]
["8.67","High",11194]
["8.68","High",11195]
["8.69","Medium",11196]
["8.7","High",8575]
["8.70","Medium",11197]
["8.71","Very High",11198]
["8.72","Medium",11199]
["8.73","Medium",11200]
["8.74","High",11201]
["8.75","Medium",11202]
["8.76","Medium",11203]
["8.77","Medium",11204]
["8.78","Medium",11205]
["8.79","Medium",11206]
["8.8","Medium",8576]
["8.80","Medium",11207]
["8.81","Low",11208]
["8.82","Medium",11209]
["8.83","Low",11210]
["8.84","Low",11211]
["8.85","Medium",11212]
["8.86","Medium",11213]
["8.87","Medium",11214]
["8.88","Low",11215]
["8.89","High",11216]
["8.9","High",8577]
["8.90","High",11217]
["8.91","High",11218]
["8.92","Medium",11219]
["8.93","Low",11220]
["8.94","Low",11221]
["8.95","Medium",11222]
["8.96","Medium",11223]
["8.97","Low",11224]
["8.98","High",11225]
["8.99","Medium",11226]
["9.1","Low",8390]
["9.10","Medium",8399]
["9.11","Medium",8400]
["9.12","Medium",8401]
["9.13","Low",8402]
["9.14","Medium",8403]
["9.15","Medium",8404]
["9.16","High",8405]
["9.17","High",8406]
["9.18","Low",8407]
["9.19","Low",8408]
["9.2","Very High",8391]
["9.20","Medium",8409]
["9.21","Medium",8410]
["9.22","Low",8411]
["9.23","Low",8412]
["9.24","Medium",8413]
["9.25","Low",8414]
["9.26","Low",8415]
["9.27","Low",8416]
["9.28","Medium",8417]
["9.29","Low",8418]
["9.3","Very High",8392]
["9.4","High",8393]
["9.5","High",8394]
["9.6","Low",8395]
["9.7","Medium",8396]
["9.8","Medium",8397]
["9.9","Medium",8398]
["9.99","High",8419]

{"sheet":"Equipment_list","index":7,"n_rows":28,"n_cols":3,"rows_kept":28,"cut":false,"hidden":true,"merged":[]}
["TITLE","Equipment_list_description","ID"]
["Accommodation",null,12]
["Cargo Mach.",null,13]
["Critical Equip.",null,16]
["Deck - Machinery",null,18]
["Deck - Mooring Machinery",null,15]
["Deck - Pipe / Fittings",null,20]
["Documentation",null,21]
["E/R - Air Comp.",null,8]
["E/R - Aux. Engine",null,4]
["E/R - Aux. Mach.",null,7]
["E/R - Boiler",null,5]
["E/R - Main Engine",null,3]
["E/R - Pipes/ valves & fittings",null,9]
["E/R - Pumps",null,32]
["E/R - Purifier",null,6]
["Elect. Mach. & Equip.",null,10]
["Hull & Tanks",null,19]
["Inert Gas",null,14]
["LSA / FFA",null,17]
["Miscellaneous",null,22]
["Navigation - DGPS / EPFS / AIS",null,28]
["Navigation - ECDIS",null,25]
["Navigation - Echo Sounder / Speed Log",null,26]
["Navigation - GMDSS & Communication",null,23]
["Navigation - Others",null,11]
["Navigation - RADAR",null,24]
["Navigation - VDR / BNWAS",null,30]

{"sheet":"PSC_MOU","index":8,"n_rows":11,"n_cols":3,"rows_kept":11,"cut":false,"hidden":true,"merged":[]}
["TITLE","PSC_MOU_description","ID"]
["Asia and the Pacific",null,2]
["Caribbean",null,4]
["Europe and the North Atlantic",null,1]
["Latin America",null,3]
["The Black Sea region",null,6]
["The Indian Ocean",null,8]
["The Mediterranean",null,7]
["The Riyadh MoU",null,9]
["USCG",null,10]
["West and Central Africa",null,5]

{"sheet":"Inspection_type","index":9,"n_rows":14,"n_cols":2,"rows_kept":14,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Bunkering Audit",14]
["Cargo Audit",17]
["Engineering Audit",16]
["ISM Audit",2]
["ISPS Audit",3]
["IT Audit",10]
["MLC Audit",1]
["Mooring Audit",9]
["Nav Audit / Verification",8]
["Onboard Training",18]
["PSC Inspection",4]
["Ship Staff Insp.",15]
["Suptd. Insp.",13]

{"sheet":"Deficiency_Cause","index":10,"n_rows":8,"n_cols":3,"rows_kept":8,"cut":false,"hidden":true,"merged":[]}
["TITLE","Deficiency_Cause_description","ID"]
["Behaviour Based",null,1]
["Equipment Related",null,4]
["External Factors",null,5]
["Human Error",null,7]
["Inappropriate Procedure",null,8]
["Industry Issue",null,6]
["Knowledge Based",null,3]

{"sheet":"Observer_code","index":11,"n_rows":3,"n_cols":3,"rows_kept":3,"cut":false,"hidden":true,"merged":[]}
["TITLE","Observer_code_description","ID"]
["Owner / Marine / Tech. Suptd.",null,3]
["Ship Staff",null,2]

{"sheet":"Status_code","index":12,"n_rows":6,"n_cols":3,"rows_kept":6,"cut":false,"hidden":true,"merged":[]}
["TITLE","Status_code_description","ID"]
["Completed",null,6]
["Deferred to D D",null,5]
["In progress",null,3]
["Not Started",null,2]
["Waiting spare",null,4]

{"sheet":"PSC_ref_no","index":13,"n_rows":19,"n_cols":2,"rows_kept":19,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Alarms",9]
["Cargo operations including equipment",7]
["Certificates & Documentation",2]
["Dangerous Goods",13]
["Emergency Systems",5]
["Fire safety",8]
["ISM",16]
["ISPS",17]
["Life saving appliances",12]
["MLC, 2006",18]
["Other",19]
["Pollution Prevention",15]
["Propulsion and auxiliary machinery",14]
["Radio communication",6]
["Safety of Navigation",11]
["Structural condition",3]
["Water/Weathertight condition",4]
["Working and Living Conditions",10]

{"sheet":"Risk_value_of_obs","index":14,"n_rows":1,"n_cols":2,"rows_kept":1,"cut":false,"hidden":true,"merged":[]}
["Risk Value of observation","ID"]

{"sheet":"Year","index":15,"n_rows":18,"n_cols":1,"rows_kept":18,"cut":false,"hidden":true,"merged":[]}
["Year"]
[2014]
[2015]
[2016]
[2017]
[2018]
[2019]
[2020]
[2021]
[2022]
[2023]
[2024]
[2025]
[2026]
[2027]
[2028]
[2029]
[2030]

{"sheet":"Month","index":16,"n_rows":13,"n_cols":1,"rows_kept":13,"cut":false,"hidden":true,"merged":[]}
["Month"]
["Jan"]
["Feb"]
["Mar"]
["Apr"]
["May"]
["Jun"]
["Jul"]
["Aug"]
["Sep"]
["Oct"]
["Nov"]
["Dec"]

{"sheet":"Date_","index":17,"n_rows":32,"n_cols":1,"rows_kept":32,"cut":false,"hidden":true,"merged":[]}
["Date"]
["01"]
["02"]
["03"]
["04"]
["05"]
["06"]
["07"]
["08"]
["09"]
[10]
[11]
[12]
[13]
[14]
[15]
[16]
[17]
[18]
[19]
[20]
[21]
[22]
[23]
[24]
[25]
[26]
[27]
[28]
[29]
[30]
[31]

{"sheet":"Sheet1","index":18,"n_rows":24,"n_cols":6,"rows_kept":24,"cut":false,"hidden":true,"merged":[]}
[]
[null,"ID","E",null,"Date Recorded",1]
[null,"UNIQUE ID","F",null,"Type of Deficiency",2]
[1,"Date Recorded","G",null,"Observer code",3]
["ignore","Vessel Type","H",null,"Type of Inspection",4]
[null,"Internal / External","I",null,"Description of Deficiency",5]
[null,"Drydock","J",null,"Equipment Categories",6]
[null,"Information Sharing","K",null,"Area of Observation",7]
[null,"Critical_item","L",null,"Deficiency Cause",8]
[null,"Deficiency Type","M",null,"VIQ Ref Number",9]
[null,"Deficiency Cause","N",null,"Risk Value of Obs",10]
[null,"Inspection Type","O",null,"PSC Ref Number",11]
[null,"Equipments","P",null,"PSC MOU ID",12]
[null,"VIQ Reference Number","Q",null,"Action Taken or Required",13]
[null,"Risk Value of the observation","R",null,"Target Date",14]
[null,"PSC Reference Number","S",null,"PO Ref No.",15]
[null,"PSC MOU","T",null,"Status Code",16]
[null,"Observer Code","U",null,"Date Completed",17]
[null,"Target Date","V",null,"Drydock",18]
[null,"Status Code","W",null,"Info Sharing",19]
[null,"Description of Deficiency","X",null,"Critical Item Flag",20]
[null,"Action taken / required","Y",null,"Audit Type",21]
[null,"PO ref no","Z"]
[null,"Date completed","AA"]

{"sheet":"Ship_information","index":19,"n_rows":2,"n_cols":4,"rows_kept":2,"cut":false,"hidden":true,"merged":[]}
["Ship_ID","Ship_Name","FILE_NAME","Export_Date"]
["55","DHT SUNDARBANS (16-04-2025)","55_1744772772254.xlsm","2025-08-28 18:08:64"]

{"sheet":"External_Deficiency_type","index":20,"n_rows":5,"n_cols":3,"rows_kept":5,"cut":false,"hidden":true,"merged":[]}
["TITLE","Type of deficiency_description","ID"]
["Condn of Class / Memo",null,5]
["Defect",null,1]
["Non Conformity",null,2]
["Observation",null,3]

{"sheet":"External_Inspection_type","index":21,"n_rows":11,"n_cols":2,"rows_kept":11,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Cargo Audit",17]
["Flag State Insp.",5]
["ISM Audit",2]
["ISPS Audit",3]
["MLC Audit",1]
["Nav Audit / Verification",8]
["OM Insp. (Eg. SIRE / CDI etc.)",6]
["Others (Eg. Insurance etc.)",12]
["PSC Inspection",4]
["Terminal Insp.",11]

{"sheet":"External_Observer_code","index":22,"n_rows":7,"n_cols":3,"rows_kept":7,"cut":false,"hidden":true,"merged":[]}
["TITLE","Observer_code_description","ID"]
["Class Surveyor",null,4]
["FSC Inspector",null,5]
["Others (Eg. Insurance etc.)",null,9]
["PSC Insp.",null,6]
["SIRE / CDI Insp.",null,8]
["Terminal Insp.",null,7]

{"sheet":"Sheet Version","index":23,"n_rows":2,"n_cols":2,"rows_kept":2,"cut":false,"hidden":true,"merged":[]}
["Version","Title"]
["2.0","Version 2.0"]