{"text_format":"1","workbook":"xlsx","n_sheets":24,"sheets":["Mainsheet","Completed","Calc","Areaofobs","Vessel_type","Deficiency_type","VIQrefno","Equipment_list","PSC_MOU","Inspection_type","Deficiency_Cause","Observer_code","Status_code","PSC_ref_no","Risk_value_of_obs","Year","Month","Date_","Sheet1","Ship_information","External_Deficiency_type","External_Inspection_type","External_Observer_code","Sheet Version"],"not_rendered":{"charts":0,"images":1,"macros":1,"external_links":0,"defined_names":12,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Mainsheet","index":0,"n_rows":19,"n_cols":28,"rows_kept":19,"cut":false,"hidden":false,"merged":[[10,8,10,9],[10,12,10,13],[12,6,12,27],[8,6,8,27]]}
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,"Defect - Damage Monitoring Sheet"]
[]
[null,null,null,null,null,null,null,"Date of Report","02-Sep-2025",null,null,"Ship Name","PERTAMINA HALMAHERA (02-07-2025)"]
[]
[null,null,null,null,null,null,"VERSION : 2.0"]
[]
[]
[]
[null,null,null,"ID","SHIPSIDE UNIQUEID","UNIQUE ID","Date Recorded","Type of Deficiency","Observer code","Type of Inspection","Description of Deficiency","Equipment Categories","Area of Observation","Deficiency Cause","VIQ Ref Number","Risk Value of Obs","PSC Ref Number","PSC MOU ID","Action Taken or Required","Target Date","PO Ref No.","Status Code","Date Completed","Drydock","Info Sharing","Critical Item","Audit Type","Superintendent Remarks"]
[null,null,null,null,52022,"106_Tue Aug 19 2025 11:22:40 GMT+0800","2025-08-19T08:00:00","Other","Ship Staff","Ship Staff Insp."," FWG 3 Way valve leaking ","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.1","Medium","",""," FWG 3 Way valve leaking from the shaft. need O ring renewal. Vessel has raised PO for same. \n PHAL250321\tFWG 3 WAY VALVE - HTV 37","2025-09-30T08:00:00"," PHAL250321","Waiting spare",null,"No","No","No","Internal"]
[null,null,null,null,52136,"106_Tue Aug 19 2025 20:27:10 GMT+0800","2025-08-12T08:00:00","Other,Breakdown","Ship Staff","Ship Staff Insp.","SCR REACTOR OUTLET BELLOW DAMAGED","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.1","Medium","","","SCR REACTOR OUTLET BELLOW ON THE EXHAST SIDE IS LEAKING AND NEED RENEWAL ","2025-09-30T08:00:00"," PHAL250323","Not Started",null,"No","No","No","Internal"]

{"sheet":"Completed","index":1,"n_rows":531,"n_cols":28,"rows_kept":531,"cut":false,"hidden":false,"merged":[[10,8,10,9],[10,12,10,13],[12,6,12,27],[8,6,8,27]]}
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,"Defect - Damage Monitoring Sheet"]
[]
[null,null,null,null,null,null,null,"Date of Report","02-Sep-2025",null,null,"Ship Name","PERTAMINA HALMAHERA (02-07-2025)"]
[]
[null,null,null,null,null,null,"VERSION : 2.0"]
[]
[]
[]
[null,null,null,"ID","SHIPSIDE UNIQUEID","UNIQUE ID","Date Recorded","Type of Deficiency","Observer code","Type of Inspection","Description of Deficiency","Equipment Categories","Area of Observation","Deficiency Cause","VIQ Ref Number","Risk Value of Obs","PSC Ref Number","PSC MOU ID","Action Taken or Required","Target Date","PO Ref No.","Status Code","Date Completed","Drydock","Info Sharing","Critical Item","Audit Type","Superintendent Remarks"]
[null,null,null,35825,10691,"106_Sat Jun 01 2024 17:43:45 GMT+0800",null,"Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Stbd pilot ladder bottom steps not strait","Miscellaneous","","","5.47","Medium","","","Stbd pilot ladder bottom steps not strait. \nLadder step straitened,","2024-03-24T23:59:35","","Completed","2024-03-16T23:59:35","No","No","No","Internal"]
[null,null,null,35829,65071,"106_Sat Jun 01 2024 17:38:23 GMT+0800",null,"Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Speaker in the forepeak store is broken from mounting","Deck - Machinery","","","","","","","To repair broken mounting for Speaker in the forepeak store. \nSpeaker placed properly. ","2024-05-02T23:59:35","","Completed","2024-04-16T23:59:35","No","No","No","Internal"]
[null,null,null,16394,null,"106_31/12/2020 2:43:58 PM","2020-07-30T23:59:35","Guarantee Claim","Ship Staff","Ship Staff Insp."," Sea water flow meter FM112 fitted on EGCS for generators not showing value. Even though enough flow is there for EGCS operation, flow meter is showing zero flow.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","PLC updation carried out and now both FM readings are matching.","2021-01-29T23:59:35","","Completed","2021-01-06T23:59:35","No","No","No","Internal"]
[null,null,null,16401,null,"106_31/12/2020 2:54:55 PM","2020-07-30T23:59:35","Guarantee Claim","Ship Staff","Ship Staff Insp.","  We have observed during running of No.2 main air compressor, at anytime we are getting MOTOR OVERLOAD alarm Error E-0080. Once you reset, compressor run and no issue, after sometime we get error E-0080 and shows MOTOR OVERLOAD alarm. There is nothing wrong with compressor and working satisfactory. We have pressed the thermal reset many times (if it got stuck) and increase the AMPS setting to 95 Amps. Still OCR is activating and giving same alarm. We suspect issue with OCR and activating at any time","E/R - Air Comp.,Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","New OCr received and renewed","2020-09-28T23:59:35","","Completed","2020-09-17T23:59:35","No","No","No","Internal"]
[null,null,null,16393,null,"106_31-Dec-20 10:02:51 AM","2020-08-09T23:59:35","Observation","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","The reference Pressure and Temperature gauges were not provided onboard for periodic comparsion of pressure and temperature gauges","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.13","Medium","","","Same was supplied onboard at Singapore on 12 Aug 2020","2020-11-09T23:59:35","","Completed","2020-08-10T23:59:35","No","No","No","External"]
[null,null,null,16402,null,"106_31-Dec-20 9:57:46 AM","2020-08-09T23:59:35","Observation","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","There was no Compound (Pressure / Vaccum) gauge provided for Cargo Sea Chest Valve testing arrangement","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","6.4","High","","","Same was immediately replaced by a Compound (Pressure / Vaccum) gauge","2020-11-09T23:59:35","","Completed","2020-08-09T23:59:35","No","No","No","External"]
[null,null,null,16403,null,"106_31-Dec-20 10:06:37 AM","2020-08-09T23:59:35","Observation","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","The acids and alkalis drums were not segregated and were stored inside the chemical locker room on top of each other on a wooden grating.","Miscellaneous","Eng. / Strg. Comp.","Human Error","10.23","Medium","","","The acids and alkalis drums were segregated and stored seperately inside the chemical locker room ","2020-11-09T23:59:35","","Completed","2020-08-10T23:59:35","No","No","No","External"]
[null,null,null,16395,null,"106_31/12/2020 3:02:21 PM","2020-08-16T23:59:35","Guarantee Claim","Ship Staff","Ship Staff Insp.","EGCS Sealing Fan no 1 casing deformed\t","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","New complete casing has been received and same has been renewed. Sealing air fan #1 tried out, no leaks observed from the casing.","2021-01-30T23:59:35","","Completed","2021-01-25T23:59:35","No","No","No","Internal"]
[null,null,null,16404,null,"106_31/12/2020 3:11:47 PM","2020-08-18T23:59:35","Guarantee Claim","Ship Staff","Ship Staff Insp.","Spring loaded valve in FW line for FWG found defective.\t","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Makers have sent new valve and and same has been renewed","2020-09-29T23:59:35","","Completed","2020-09-11T23:59:35","No","No","No","Internal"]
[null,null,null,16405,null,"106_31/12/2020 3:16:11 PM","2020-08-20T23:59:35","Guarantee Claim","Ship Staff","Ship Staff Insp.","BWTS Hydrogen sensor not working","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","New hydrogen sensor has been received and replaced and working fine now","2020-11-28T23:59:35","","Completed","2020-11-18T23:59:35","No","No","No","Internal"]
[null,null,null,17316,null,"106_04-01-2021 17:11:00","2020-08-23T23:59:35","Guarantee Claim","Ship Staff","Ship Staff Insp.","Aux boiler HFO flowmeter for both boilers found not working.\t\t","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Makers advised for software upgrade, same done by service engineer at singapore on 29thdec2020. Vessel changed over to HFO on 2jan 2021 after departure singapore. Observed HFO flowmeter operational. ","2021-01-13T23:59:35","GC007","Completed","2020-12-31T23:59:35","No","No","No","Internal"]
[null,null,null,17317,null,"106_04-01-2021 17:15:47","2020-08-30T23:59:35","Guarantee Claim","Ship Staff","Ship Staff Insp.","Fresh water Generator high salinity alarm due to faulty non return valve.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Spare received under GC and Spare NRV fitted. FWG operational.","2020-12-29T23:59:35","GC008","Completed","2020-09-11T23:59:35","No","No","No","Internal"]
[null,null,null,17318,null,"106_04-01-2021 17:21:58","2020-08-30T23:59:35","Guarantee Claim","Ship Staff","Ship Staff Insp.","Fresh water Generator Solenoid valve found faulty ","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Spare solenoid received under gc renewed. FWG working satisfactory","2020-12-29T23:59:35","GC009","Completed","2020-09-11T23:59:35","No","No","No","Internal"]
[null,null,null,17319,null,"106_04-01-2021 17:35:01","2020-09-05T23:59:35","Guarantee Claim","Ship Staff","Ship Staff Insp.","Main air Compressor No:2 OCR relay found faulty\t","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","OCR relay renewed with new spare, Compressor operationing satisfactory","2020-11-28T23:59:35","GC011","Completed","2020-10-24T23:59:35","No","No","No","Internal"]
[null,null,null,17320,null,"106_04-01-2021 17:30:10","2020-09-05T23:59:35","Guarantee Claim","Ship Staff","Ship Staff Insp.","Elevator counterweight guide rail metal shavings at various locations. Guide shoes inspected found to be worn out .","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Maker SE attended the vessel at SG and repair work carried out. Problem rectified.","2021-01-29T23:59:35","","Completed","2020-12-27T23:59:35","No","No","No","Internal"]
[null,null,null,17321,null,"106_04-01-2021 17:57:54","2020-09-06T23:59:35","Guarantee Claim","Ship Staff","Ship Staff Insp.","Control air compressor Auto drain solenoid valve found inoperational. \t","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Spare valve received and renewed. Solenoid valve operational satisfactory. Spare received under GC kept as spare. ","2020-12-29T23:59:35","GC012","Completed","2020-12-27T23:59:35","No","No","No","Internal"]
[null,null,null,16406,null,"106_31-Dec-20 9:04:29 AM","2020-09-09T23:59:35","Observation","Ship Staff","Nav Audit / Verification","VDR Data retrieving software not installed onobard","Navigation - VDR / BNWAS","Navigation","Human Error","4.7","High","","","The software was downloaded on the Nav PC and checked by downloading from the VDR. Observed the VDR Playback to be satisfactory","2020-12-09T23:59:35","","Completed","2020-09-21T23:59:35","No","No","No","Internal"]
[null,null,null,16407,null,"106_31-Dec-20 9:07:53 AM","2020-09-09T23:59:35","Observation","Ship Staff","Nav Audit / Verification","ECDIS Failure drill not conducted with Office","Navigation - ECDIS","Navigation","Inappropriate Procedure","4.7","High","","","ECDIS Failure drill carried out with Office","2020-12-09T23:59:35","","Completed","2020-11-17T23:59:35","No","No","No","Internal"]
[null,null,null,16408,null,"106_31-Dec-20 9:11:40 AM","2020-09-09T23:59:35","Observation","Ship Staff","Nav Audit / Verification","Initial found missing at some corrections in Bridge Bell book","Documentation","ISM Related","Human Error","4.2","Medium","","","All corrections where the Initial were missing were signed by the respective Officers","2020-12-09T23:59:35","","Completed","2020-09-21T23:59:35","No","No","No","Internal"]
[null,null,null,16409,null,"106_31-Dec-20 8:13:33 AM","2020-09-10T23:59:35","Guarantee Claim","Ship Staff","Ship Staff Insp.","Steering Gear – Auto pilot control box timers faulty resulting in Steering failure from the Bridge","Navigation - Others","Navigation","Equipment Related","4.7","High","","","2 nos faulty timers replaced with spare timers received at Lome","2020-12-09T23:59:35","","Completed","2020-10-25T23:59:35","No","No","No","Internal"]
[null,null,null,17322,null,"106_04-01-2021 18:09:26","2020-09-12T23:59:35","Guarantee Claim","Ship Staff","Ship Staff Insp.","LO Drain tank local level guage found faulty","Hull & Tanks","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Makers advice received and zero calibration carried out. Tank guage working in order.","2020-11-28T23:59:35","GC014","Completed","2020-11-04T23:59:35","No","No","No","Internal"]
[null,null,null,17305,null,"106_04-01-2021 18:16:51","2020-09-13T23:59:35","Guarantee Claim","Ship Staff","Ship Staff Insp.","EGCS water analyzer sampling pipe to be renewed as present installation is plastic.\t","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","PVC pipe and fittings spare received .EGCS water analyzer sampling pipe renewed with PVC pipe .","2021-06-28T23:59:35","GC015","Completed","2021-05-16T23:59:35","No","No","No","Internal"]
[null,null,null,17323,null,"106_04-01-2021 18:20:51","2020-09-16T23:59:35","Guarantee Claim","Ship Staff","Ship Staff Insp.","Incinerator Emergency stop switch in ecr panel found not operational.\t","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Spare received and Emergency stop switch renewed. Inicinerator operational and emergency stop working satisfactory.","2020-11-28T23:59:35","GC016","Completed","2020-11-04T23:59:35","No","No","No","Internal"]
[null,null,null,17324,null,"106_04-01-2021 18:32:44","2020-10-05T23:59:35","Guarantee Claim","Ship Staff","Ship Staff Insp.","Quick closing devices- Pressure reducing valve found to be leaking. PRV valve seat found damaged.","Critical Equip.","Safety / LSA / FFA","Equipment Related","10.17","Very High","","","Spare PRV valve replaced, No leaks from PRV","2020-11-28T23:59:35","GC018","Completed","2020-11-12T23:59:35","No","No","No","Internal"]
[null,null,null,17325,null,"106_04-01-2021 18:36:10","2020-10-08T23:59:35","Guarantee Claim","Ship Staff","Ship Staff Insp.","HFO Transfer pump - minor leaks from mechanical seal\t","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Spare mechanical sea received. no leaks observed from the pum","2020-12-29T23:59:35","GC019","Completed","2020-11-04T23:59:35","No","No","No","Internal"]
[null,null,null,17326,null,"106_04-01-2021 18:42:56","2020-10-09T23:59:35","Guarantee Claim","Ship Staff","Ship Staff Insp.","Diary room Thermometer found defective\t","Accommodation","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Spare received and thermometer renewed. ","2020-12-29T23:59:35","GC020","Completed","2020-11-04T23:59:35","No","No","No","Internal"]
[null,null,null,17327,null,"106_04-01-2021 18:50:20","2020-10-09T23:59:35","Guarantee Claim","Ship Staff","Ship Staff Insp.","Oily bilge separator pump fresh water inlet valve bonnet found broken. \t","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Spare bonnet received under GC renewed. ","2020-12-29T23:59:35","GC021","Completed","2020-11-04T23:59:35","No","No","No","Internal"]
[null,null,null,16396,null,"106_31-Dec-20 8:34:20 AM","2020-10-12T23:59:35","Guarantee Claim","Ship Staff","Ship Staff Insp.","Mooring Winch Brake testing kit Hydraulic Hand Pump faulty","Deck - Mooring Machinery","Mooring","Equipment Related","9.7","Medium","","","Spare pump received and testing carried out.","2021-01-12T23:59:35","GC-022-DECK","Completed","2021-01-02T23:59:35","No","No","No","Internal"]
[null,null,null,17328,null,"106_05-01-2021 00:16:59","2020-10-13T23:59:35","Guarantee Claim","Ship Staff","Ship Staff Insp.","CCTV camera in midship manifold area found not working. Blank screen display in monitor","Miscellaneous","General Appearance","Equipment Related","","","","","Spare camera received same renewed. All ship CCTV camera working in order","2020-12-29T23:59:35","","Completed","2020-11-21T23:59:35","No","No","No","Internal"]
[null,null,null,16397,null,"106_31-Dec-20 8:40:14 AM","2020-10-18T23:59:35","Guarantee Claim","Ship Staff","Ship Staff Insp.","The F – Spanners provided along with the Fire and Foam Hydrants are Big in size and do not fit the Wheel of the Fire and Foam Hydrant","LSA / FFA","Safety / LSA / FFA","Equipment Related","12.15","High","","","Received and put in use.","2021-01-17T23:59:35","GC-025-DECK","Completed","2020-12-30T23:59:35","No","No","No","Internal"]
[null,null,null,16398,null,"106_31-Dec-20 10:12:17 AM","2020-10-28T23:59:35","Observation","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","Records were not available for Pressure comparsion of Cargo tanks as vessel was not provided with portable manometer","Inert Gas","Cargo / Ballast Systems","Equipment Related","8.13","Medium","","","Portable manometer supplied at Fujairah this call. Manometer fitting properly and verified proper functioning.","2021-01-28T23:59:35","BCIA200053","Completed","2021-01-28T23:59:35","No","No","No","External"]
[null,null,null,16410,null,"106_31-Dec-20 9:27:00 AM","2020-10-29T23:59:35","Observation","Owner / Marine / Tech. Suptd.","MLC Audit","Hospital bath tub - recommend place naphthene balls in the drain to prevent foul smell","Accommodation","MLC Related","Human Error","11.15","Low","","","Few Naphthalene balls placed above the bath tub drain as per the recommendation","2020-12-29T23:59:35","","Completed","2020-11-02T23:59:35","No","No","No","Internal"]
[null,null,null,16411,null,"106_31-Dec-20 9:29:41 AM","2020-10-29T23:59:35","Observation","Owner / Marine / Tech. Suptd.","MLC Audit","Hospital bed - did not sight any securing arrangements in heavy weather conditions","Accommodation","MLC Related","Equipment Related","11.15","Low","","","The bed was secured towards bulk head using screws on its two supports . Bed was tested applying force to the extent to move it in unsecured condition or in heavy weather. found secured and not movable in heavy weather condition","2020-12-29T23:59:35","","Completed","2020-11-02T23:59:35","No","No","No","Internal"]
[null,null,null,16412,null,"106_31-Dec-20 9:39:00 AM","2020-10-29T23:59:35","Observation","Owner / Marine / Tech. Suptd.","ISM Audit","Sprinkler system and valve for the Mast riser was not Marked and stencilled","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.4","High","","","Sprinkler system line and valves of the mastriser painted red and stenciled for proper identification, IMO symbol posted","2020-12-29T23:59:35","","Completed","2020-11-02T23:59:35","No","No","No","Internal"]
[null,null,null,16413,null,"106_31-Dec-20 9:42:25 AM","2020-10-29T23:59:35","Observation","Owner / Marine / Tech. Suptd.","ISM Audit","Some flanges in the Hydraulic lines of Forward Hydraulic power pack were not covered with Anti splash tapes\n\nin Foscle store","Deck - Mooring Machinery","Mooring","Equipment Related","10.23","Medium","","","Installed Anti splash tape on the missing anti splash tape flanges in the Bosun store","2020-12-29T23:59:35","","Completed","2020-11-01T23:59:35","No","No","No","Internal"]
[null,null,null,16414,null,"106_31-Dec-20 9:45:20 AM","2020-10-29T23:59:35","Non Conformity","Owner / Marine / Tech. Suptd.","ISM Audit","Support stanchions missing in the Steering Gear Room walkway","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.43","Medium","","","As soon as this was identified, same was brought to the notice of Top management and as a immediate corrective action, area was cordoned off and a safety poster put in place. Matter was discussed in the closing tool box meeting and all crew made aware of the safety lapse on the SG platform","2020-12-29T23:59:35","","Completed","2020-10-31T23:59:35","No","No","No","Internal"]
[null,null,null,16415,null,"106_31-Dec-20 9:48:27 AM","2020-10-29T23:59:35","Observation","Owner / Marine / Tech. Suptd.","ISM Audit","Poster at the entrance of ER stated that the machinery spaces is provided with Gas Flooding system. Whereas the fixed fire fighting system for the ER is High Expansion Foam","LSA / FFA","Eng. / Strg. Comp.","Human Error","5.4","High","","","IMO poster was amended with Dymo tape and correct fire fighting medium was printed on the poster. This was identified for all the spaces and changed","2020-12-29T23:59:35","","Completed","2020-10-30T23:59:35","No","No","No","Internal"]
[null,null,null,16417,null,"106_31-Dec-20 9:35:02 AM","2020-10-29T23:59:35","Observation","Owner / Marine / Tech. Suptd.","ISM Audit","Some Gratings in the Pumproom Bottom are having raised frames which present a Tripping hazard","Miscellaneous","Structural Condn. / WT integrity ","Equipment Related","5.47","Medium","","","All uneven gratings in the Pumproom highlighted with yellow colors to caution the personnel to avoid trip and fall","2020-12-29T23:59:35","","Completed","2020-11-01T23:59:35","No","No","No","Internal"]
[null,null,null,17329,null,"106_05-01-2021 00:44:47","2020-11-25T23:59:35","Guarantee Claim","Ship Staff","Ship Staff Insp.","ME Intermediate shaft bearing - Shaft pass cover sealing ring found in oil sump","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Wartsila SE attended and carried out inspection and repair.","2021-01-29T23:59:35","","Completed","2021-01-11T23:59:35","No","No","No","Internal"]
[null,null,null,16399,null,"106_31-Dec-20 8:47:22 AM","2020-12-05T23:59:35","Guarantee Claim","Ship Staff","Ship Staff Insp.","During weekly inspection of Lifeboats it was observed that one of the connection hose from the air bottle of Starboard Lifeboat was leaking","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.29","High","","","Hose renewed","2021-03-04T23:59:35","GC-027-DECK","Completed","2021-01-01T23:59:35","No","No","No","Internal"]
[null,null,null,16400,null,"106_31-Dec-20 8:53:29 AM","2020-12-05T23:59:35","Guarantee Claim","Ship Staff","Ship Staff Insp.","Vessel has identified around 12 hydraulic valves in Pumproom & P/room Void space which are leaking from the O-Ring","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.21","High","","","All leaking valve OR's have been changed.No more leaks now ","2021-03-04T23:59:35","GC-028-DECK","Completed","2021-01-10T23:59:35","No","No","No","Internal"]
[null,null,null,17330,null,"106_05-01-2021 01:02:47","2020-12-05T23:59:35","Guarantee Claim","Ship Staff","Ship Staff Insp.","ME & AE FCM unit cv-4 valve issue\t","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Alfa laval service engineer attended vessel in singapore. Upgraded software for HMI & PLC by service engineer. CV-4 operational when changing over to HFO from MGO. CV4 operational now ","2021-01-29T23:59:35","","Completed","2021-01-12T23:59:35","No","No","No","Internal"]
[null,null,null,17306,null,"106_5/1/2021 5:32:13 PM","2020-12-06T23:59:35","Guarantee Claim","Ship Staff","Ship Staff Insp.","EGCS system noise interference with MF-HF Alarm testing","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","EGCSC system software updated as per maker instruction due to which delay time increased  for perticular pressure transmiter and MF-HF alarm problem solved.","2021-07-28T23:59:35","GC-030","Completed","2021-05-05T23:59:35","No","No","No","Internal"]
[null,null,null,16416,null,"106_31-Dec-20 8:25:02 AM","2020-12-12T23:59:35","Guarantee Claim","Ship Staff","Ship Staff Insp.","The dimmer for the ME RPM indicator on the Bridge overhead console not working","Navigation - Others","Navigation","Equipment Related","4.7","High","","","Same is replaced with new RPM indicator received in Singapore on 29 Dec 2020","2021-03-11T23:59:35","","Completed","2020-12-29T23:59:35","No","No","No","Internal"]
[null,null,null,17331,null,"106_10-01-2021 16:56:33","2020-12-14T23:59:35","Guarantee Claim","Ship Staff","Ship Staff Insp.","Garbage compactor inoperational.","Elect. Mach. & Equip.","General Appearance","Equipment Related","6.2","High","","","Garbage compactor found not working, suspected plc malfunction. makers supplied plc under GC. Upon further investigation found truch limit switch not making contact internally, same rectified, compactor working satisfactory","2021-01-29T23:59:35","GC032","Completed","2020-12-27T23:59:35","No","No","No","Internal"]
[null,null,null,17307,null,"106_10-01-2021 17:03:59","2020-12-16T23:59:35","Guarantee Claim","Ship Staff","Ship Staff Insp.","Excessive vibration observed in ER SCR platform at vessel loaded condition between 58-61 rpm\t","Hull & Tanks","Eng. / Strg. Comp.","Equipment Related","11.5","Medium","","","GC raised and communication with yard in progress. Videos and photos sent to yard for analysing.Yard Already despatched materials to arrest the vibrations ,Awaiting supply on board ","2021-12-29T23:59:35","GC-033","Completed","2021-11-09T23:59:35","No","No","No","Internal"]
[null,null,null,17332,null,"106_10-01-2021 17:13:26","2020-12-16T23:59:35","Guarantee Claim","Ship Staff","Ship Staff Insp.","Inert gas genertor main burner solenoid valve found defective.\t","E/R - Aux. Mach.,Inert Gas","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","New spare solenoid valve renewed. IGG operational.  GC raised and vessel received new solenoid valve which is kept as spare.","2021-01-29T23:59:35","GC035","Completed","2020-12-27T23:59:35","No","No","No","Internal"]
[null,null,null,17333,null,"106_10-01-2021 17:07:44","2020-12-16T23:59:35","Guarantee Claim","Ship Staff","Ship Staff Insp.","Deck flood lights water ingress due to poor quality fittings.","Elect. Mach. & Equip.","General Appearance","Equipment Related","11.11","Very High","","","Spare light fittings received and renewed. All repairs also carried out.","2021-01-29T23:59:35","","Completed","2021-01-13T23:59:35","No","No","No","Internal"]
[null,null,null,17308,null,"106_10-01-2021 17:16:52","2020-12-21T23:59:35","Guarantee Claim","Ship Staff","Ship Staff Insp.","EGCS SW pump VFD issue\t","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","EGCS SW pump VFD is kept in auto mode but observed it is not modulating its frequency as per requirements. Communication with makers in progress.","2021-12-29T23:59:35","GC036","Completed","2021-11-09T23:59:35","No","No","No","Internal"]
[null,null,null,17310,null,"106_10-01-2021 17:20:14","2020-12-21T23:59:35","Guarantee Claim","Ship Staff","Ship Staff Insp.","EGCS operational issues","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","EGCS service engineer attained , software updated, EGCS operational issue solved.","2021-07-29T23:59:35","GC037","Completed","2021-05-08T23:59:35","No","No","No","Internal"]
[null,null,null,17304,null,"106_11-01-2021 03:33:04","2020-12-27T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Varnish not done on small valve plates on deck to be carried out\t","Deck - Pipe / Fittings","General Appearance","Knowledge Based","11.3","Medium","","","Varnish to be applied on valve plates","2021-01-27T23:59:35","","Completed","2021-01-21T23:59:35","No","No","No","Internal"]
[null,null,null,17309,null,"106_10-01-2021 17:32:53","2020-12-27T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Weeping signs seen on louvres of funne. Same to be removed and painted","Hull & Tanks","General Appearance","Knowledge Based","11.8","Low","","","Weeping signs on EGCS funnel removed and painting carried out. ","2021-01-27T23:59:35","","Completed","2021-01-24T23:59:35","No","No","No","Internal"]
[null,null,null,17311,null,"106_11-01-2021 03:28:19","2020-12-27T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Steam valve trays area near port side manifold near IG supply to 4COT(s) can be seen with rust spots. Same to be de-rusted and painted","Deck - Pipe / Fittings","General Appearance","Knowledge Based","11.3","Medium","","","De-rusting and painting to be carried out.","2021-01-27T23:59:35","","Completed","2021-01-21T23:59:35","No","No","No","Internal"]
[null,null,null,17312,null,"106_11-01-2021 15:10:00","2020-12-27T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Rust has started appearing on windlass. Same to be attended and plates to be varnished","Deck - Mooring Machinery","Mooring","Equipment Related","9.14","Medium","","","derusting and painting to be carried out.","2021-02-13T23:59:35","","Completed","2021-01-20T23:59:35","No","No","No","Internal"]
[null,null,null,17313,null,"106_11-01-2021 16:35:26","2020-12-27T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Permanent stand for pipes and plates to be fabricated as proposed in the steering flat","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Knowledge Based","11.4","Very High","","","Permanent stand for pipes not technically feasible in steering gear compartment due to close proximity of FW tanks and AFT peak tank. Damage to the internal paint coating can happen. Same discussed with suptd and pipe stand not fabricated.","2021-03-27T23:59:35","","Completed","2021-03-18T23:59:35","No","No","No","Internal"]
[null,null,null,17314,null,"106_11-01-2021 16:51:03","2020-12-27T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","EGCS room Louvre arrangement to be modified as water is seeping in when it is raining outside.","Miscellaneous","Eng. / Strg. Comp.","Knowledge Based","10.32","Very High","","","Arrangement for water seepage made in EGCs room louvres. Permanent conversion of louvres to be proposed during next drydock.","2021-03-27T23:59:35","","Completed","2021-02-08T23:59:35","No","No","No","Internal"]
[null,null,null,17315,null,"106_11-01-2021 16:54:10","2020-12-27T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Funnel stack to be painted as rust spots can be observed","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Funnel stacks de rusted and painted for both Main and EGCS funnel stacks.","2021-01-27T23:59:35","","Completed","2021-01-25T23:59:35","No","No","No","Internal"]
[null,null,null,17334,null,"106_10-01-2021 19:17:59","2020-12-27T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Stripping in accomodation area to be done properly. Some areas found dirty\t","Accommodation","General Appearance","Knowledge Based","11.13","Low","","","Stripping and waxing of accomodation decks and common places carried out.","2021-01-13T23:59:35","","Completed","2021-01-02T23:59:35","No","No","No","Internal"]
[null,null,null,17335,null,"106_10-01-2021 19:30:18","2020-12-27T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Spare Anchor to be given a fresh coat of paint.\t","Miscellaneous","General Appearance","Knowledge Based","9.2","Very High","","","Painting of spare anchor carried out.","2021-02-13T23:59:35","","Completed","2021-01-06T23:59:35","No","No","No","Internal"]
[null,null,null,17336,null,"106_11-01-2021 16:26:09","2020-12-27T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Date for oxygen and acetylene flash back arrestor to be stencilled","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","5.26","Medium","","","flashback arrestor date stenciled.","2021-01-11T23:59:35","","Completed","2021-01-02T23:59:35","No","No","No","Internal"]
[null,null,null,17337,null,"106_11-01-2021 16:32:15","2020-12-27T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Greasing of boiler safety valve wire to be carried out.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Greasing of safety valve wire, guage glass wires carried out.","2021-01-03T23:59:35","","Completed","2021-01-02T23:59:35","No","No","No","Internal"]
[null,null,null,17338,null,"106_11-01-2021 16:38:42","2020-12-27T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","EGCS SW pump no2 sacrificial flange found leaking\t","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Flange tightened, no leaks observed","2021-01-13T23:59:35","","Completed","2021-01-01T23:59:35","No","No","No","Internal"]
[null,null,null,17339,null,"106_11-01-2021 16:44:41","2020-12-27T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Waste oil tank steam heating inlet line found leaking from flange. Same to be rectified.\t","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.29","Medium","","","Flange tightened, no leaks observed.","2021-01-13T23:59:35","","Completed","2021-01-01T23:59:35","No","No","No","Internal"]
[null,null,null,17340,null,"106_11-01-2021 16:59:18","2020-12-27T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Electrical mattings found missing at some locations at the local starter panels.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.24","Low","","","Electrical insultion mats at local starter panels were put/replaced as necessary","2021-01-03T23:59:35","","Completed","2021-01-02T23:59:35","No","No","No","Internal"]
[null,null,null,17341,null,"106_11-01-2021 17:02:03","2020-12-27T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Precautions to be taken during ME fuel testing to be posted in the testing room.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","ME fuel test device procedure, Fuel test pressure, precaution poster posted at the ME fuel testing room","2021-01-03T23:59:35","","Completed","2021-01-01T23:59:35","No","No","No","Internal"]
[null,null,null,17342,null,"106_10-01-2021 17:58:43","2020-12-27T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Galley fridge and containers arrangements to be improved and be made more systematic\t","Accommodation","General Appearance","Behaviour Based,Human Error","11.13","Low","","","Rectified","2021-01-27T23:59:35","","Completed","2020-12-30T23:59:35","No","No","No","Internal"]
[null,null,null,17343,null,"106_10-01-2021 19:26:41","2020-12-27T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","High level alarm board on top of bridge front to be cleaned.","Miscellaneous","General Appearance","Knowledge Based","11.8","Low","","","High level alarm board cleaned","2021-01-13T23:59:35","","Completed","2021-01-06T23:59:35","No","No","No","Internal"]
[null,null,null,17344,null,"106_10-01-2021 19:23:12","2020-12-27T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Food seen lying open in the pantry. This practice should be stopped with immediate effect.","Accommodation","General Appearance","Behaviour Based","11.13","Low","","","Galley staffs instructed to be keep all food items covered at all times. Pantry cleaned and arranged accordingly. ","2020-12-29T23:59:35","","Completed","2020-12-28T23:59:35","No","No","No","Internal"]
[null,null,null,17345,null,"106_11-01-2021 15:06:45","2020-12-27T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Denso tape at many locations on crane hoses is peeling off.","Deck - Machinery","General Appearance","Equipment Related","8.76","Medium","","","Denso tape renewed","2021-01-27T23:59:35","","Completed","2021-01-07T23:59:35","No","No","No","Internal"]
[null,null,null,17346,null,"106_11-01-2021 16:29:33","2020-12-27T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ME TC filter manometer to be renewed as cracked. Liquid to be colored for easy identification.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Manometer repaired and color liquid added for ease of identification","2021-02-13T23:59:35","","Completed","2020-12-30T23:59:35","No","No","No","Internal"]
[null,null,null,18750,null,"106_02-02-2021 04:43:48","2021-01-23T23:59:35","Guarantee Claim","Ship Staff","Ship Staff Insp.","Fixed gas detection system solenoid valve faulty on Inert gas pipe between scrubber and deck seal\t","Deck - Machinery","Eng. / Strg. Comp.","Equipment Related","5.21","Medium","","","Fulty solinoid replaced with onboard spare and received GC-spares kept as ST bY spare. System is operational.","2021-07-29T23:59:35","GC040","Completed","2021-02-23T23:59:35","No","No","No","Internal"]
[null,null,null,18769,null,"106_02-02-2021 04:32:54","2021-01-23T23:59:35","Guarantee Claim","Ship Staff","Ship Staff Insp.","Incinerator main burner pressure gauge for oil inlet found defective","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","GC raised for new pressure gauge. Renewed with spare pressure gauge kept onboard. New pressure gauge will be supplied under GC","2021-03-28T23:59:35","GC038","Completed","2021-01-24T23:59:35","No","No","No","Internal"]
[null,null,null,18770,null,"106_02-02-2021 04:36:48","2021-01-23T23:59:35","Guarantee Claim","Ship Staff","Ship Staff Insp.","High Expansion foam pump Ammeter found not working \t","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","GC raised, adjustments made as per maker advise, ammeter working in order.","2021-03-29T23:59:35","GC039","Completed","2021-01-27T23:59:35","No","No","No","Internal"]
[null,null,null,18771,null,"106_02-02-2021 04:48:05","2021-01-27T23:59:35","Guarantee Claim","Ship Staff","Ship Staff Insp.","Shaft earthing device brush holder found defective, not holding the silver graphite brush in place. Due to which shaft earthing monitoring device gives alarm.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Spare received and replaced. Working satisfactory","2021-03-29T23:59:35","GC041","Completed","2021-02-16T23:59:35","No","No","No","Internal"]
[null,null,null,18751,null,"106_16-03-2021 09:48:16","2021-02-01T23:59:35","Guarantee Claim","Ship Staff","Ship Staff Insp.","Safety hoop not provide on various ER vertical ladders ","Miscellaneous","Eng. / Strg. Comp.","Knowledge Based","12.9","High","","","Awaiting supply of spares ","2021-12-29T23:59:35","GC-042","Completed","2021-11-09T23:59:35","No","No","No","Internal"]
[null,null,null,18749,null,"106_16-03-2021 10:10:09","2021-02-06T23:59:35","Guarantee Claim","Ship Staff","Ship Staff Insp.","Service air compressor coolant filter","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Coolant filter renewed with spare onboard,awaiting spare received kept as st by spare.","2021-05-29T23:59:35","GC-043","Completed","2021-05-11T23:59:35","No","No","No","Internal"]
[null,null,null,18752,null,"106_16-03-2021 10:18:57","2021-02-25T23:59:35","Guarantee Claim","Ship Staff","Ship Staff Insp.","HFO Purifier No 1 Belt driving device Bearing damaged","E/R - Purifier","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Bearing has been replaced with spare available onboard, received spare kept as st by spare.","2021-05-29T23:59:35","GC-044","Completed","2021-05-11T23:59:35","No","No","No","Internal"]
[null,null,null,18753,null,"106_16-03-2021 10:26:07","2021-03-02T23:59:35","Guarantee Claim","Ship Staff","Ship Staff Insp.","Engine control console exhaust fan temperature switch defective","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Engine control console exhaust fan with temeperature switch complete spare received and fiited in Engine control console. working good. ","2021-05-29T23:59:35","GC-045","Completed","2021-05-10T23:59:35","No","No","No","Internal"]
[null,null,null,18754,null,"106_16-03-2021 10:30:14","2021-03-02T23:59:35","Guarantee Claim","Ship Staff","Ship Staff Insp.","Stern Tube LO Pump no 2 RH meter faulty","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Stern Tube LO Pump no 2 RH meter spare received and fitted in place , working good.","2021-05-29T23:59:35","GC-046","Completed","2021-05-10T23:59:35","No","No","No","Internal"]
[null,null,null,18755,null,"106_16-03-2021 10:39:25","2021-03-03T23:59:35","Guarantee Claim","Ship Staff","Ship Staff Insp.","EGCS Gas Analyzer Unit Data Extraction Issue","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","EGCS  Gas Analyzer Unit Data Extraction Issue solved by service engineer. EGCS data extracted from ME and AE GAS sampling unit and stored in ships computer.","2021-05-13T23:59:35","GC-047","Completed","2021-05-08T23:59:35","No","No","No","Internal"]
[null,null,null,18756,null,"106_16-03-2021 10:45:17","2021-03-04T23:59:35","Guarantee Claim","Ship Staff","Ship Staff Insp.","Main Switch Board AE #2 ACB LED indication faulty","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Faulty LED was replaced with spare LED onboard.Received spare kept as St By spare.","2021-05-29T23:59:35","GC-048","Completed","2021-05-11T23:59:35","No","No","No","Internal"]
[null,null,null,18757,null,"106_16-03-2021 10:48:08","2021-03-04T23:59:35","Guarantee Claim","Ship Staff","Ship Staff Insp.","Aux Engine FCM Thermometer faulty","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Aux Engine FCM Thermometer spare received and fitted in place , working good.","2021-05-29T23:59:35","GC-049","Completed","2021-05-11T23:59:35","No","No","No","Internal"]
[null,null,null,18758,null,"106_16-03-2021 10:51:35","2021-03-06T23:59:35","Guarantee Claim","Ship Staff","Ship Staff Insp.","EGCS Inlet Water Analyzing Unit pH sensor faulty","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","As per makers sensor kept dry, GC not covered. Vessel renewed pH sensor from spare. ","2021-11-28T23:59:35","GC-050","Completed","2021-03-15T23:59:35","No","No","No","Internal"]
[null,null,null,18759,null,"106_16-03-2021 10:54:38","2021-03-06T23:59:35","Guarantee Claim","Ship Staff","Ship Staff Insp.","Pressure Gauge on Fire Line In-operational","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Pressure gauge replaced with spare available onboard.Awaiting spare from maker.","2021-05-29T23:59:35","GC-051","Completed","2021-05-08T23:59:35","No","No","No","Internal"]
[null,null,null,18760,null,"106_16-03-2021 10:57:56","2021-03-06T23:59:35","Guarantee Claim","Ship Staff","Ship Staff Insp.","Galley Dish washer boiler thermostat switch faulty","Accommodation","General Appearance","Equipment Related","11.13","Low","","","Galley Dish washer boiler thermostat switch spare received and fitted in place . Galley dish washer boiler tried out , working good.","2021-05-29T23:59:35","GC-052","Completed","2021-05-11T23:59:35","No","No","No","Internal"]
[null,null,null,18761,null,"106_17/4/2021 12:49:46 AM","2021-03-12T23:59:35","Guarantee Claim","Ship Staff","Ship Staff Insp.","No.1 Port Cargo manifold pressure transmitter Faulty. Showing wrong reading","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.13","Medium","","","Spare pressure Transmitter received same fitted and calibrated found working ok . Monitored during cargo discharging operation at Algeciras found working good","2021-06-12T23:59:35","GC-054","Completed","2021-08-03T23:59:35","No","No","No","Internal"]
[null,null,null,18762,null,"106_17/4/2021 12:55:10 AM","2021-03-14T23:59:35","Guarantee Claim","Ship Staff","Ship Staff Insp.","MGO transfer pump Suction pressure gauge faultynot showing correct value .","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","MGO transfer pump Suction pressure gauge spare received and faulty pressure gauge renewed.working good.","2021-06-14T23:59:35","GC-055","Completed","2021-05-13T23:59:35","No","No","No","Internal"]
[null,null,null,18763,null,"106_17/4/2021 4:50:29 AM","2021-03-16T23:59:35","Guarantee Claim","Ship Staff","Ship Staff Insp.","AE scr urea pump unit discharge chamber found leaking , hair line crack observed on weld seam.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Replacement Spare received from Maker on 18th June and kept as spare St. By","2021-06-28T23:59:35","GC-056","Completed","2021-06-16T23:59:35","No","No","No","Internal"]
[null,null,null,19662,null,"106_15/6/2021 4:39:15 AM","2021-03-18T23:59:35","Observation","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","Monkey Island \"Sailor Cobham\" V-Sat System. The microwave radiation minimum safe distance was observed designated as thirty (30) metres. No warning sign was observed upon accessing to the Monkey Island Deck. In addition, the existing safety line painted on deck was observed stenciled approx. 2.0 meters away from the antenna","Elect. Mach. & Equip.","Communication","Equipment Related","11.1","High","","","Warning Sign has been permanently marked at access to the compass deck, highlighting the danger and caution that V-SAT to be switched off prior access to the Compass Deck. \n\nAlso, the existing safety line on compass deck erased from location. \n\n\n\nAll ship’s compliment briefed on the existing Hazard and ship specific procedures established to switch off the V-SAT, prior access to Compass deck is required.","2021-04-18T23:59:35","NA","Completed","2021-03-22T23:59:35","No","No","No","External"]
[null,null,null,19663,null,"106_15/6/2021 4:13:28 AM","2021-03-28T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Doppler Speed Log showing incorrect speed on Bottom tracking. Also, Repeaters in wheelhouse and bridge wings not following the main display. ","Navigation - Echo Sounder / Speed Log","Navigation","Equipment Related","4.7","High","","","Trouble shooting carried out with Office and Maker - Software Upgraded and Reference Point Calibration carried out. ","2021-06-28T23:59:35","NA","Completed","2021-04-27T23:59:35","No","No","No","Internal"]
[null,null,null,22239,null,"106_30-10-2021 07:31:41","2021-03-30T23:59:35","Observation","Ship Staff","Ship Staff Insp.","MOB release pin found jammed.","LSA / FFA","Safety / LSA / FFA","Behaviour Based","5.31","High","","","MOB release pin maintenance carried out and freed for smooth operation in case of Man Overboard.","2021-04-13T23:59:35","","Completed","2021-04-13T23:59:35","No","No","No","Internal"]
[null,null,null,22240,null,"106_30-10-2021 07:33:48","2021-03-30T23:59:35","Observation","Ship Staff","Ship Staff Insp.","All mushroom vents identification istensils are missing.","Deck - Machinery","General Appearance","Knowledge Based","11.7","High","","","All mushroom vents identification markings stencilled permanently.","2021-05-13T23:59:35","","Completed","2021-05-12T23:59:35","No","No","No","Internal"]
[null,null,null,22241,null,"106_30-10-2021 07:37:11","2021-03-30T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Laundry ducts outside accommodation to be clean and PMS routine to be added for same.","Accommodation","General Appearance","Human Error","11.8","Low","","","Laundry ducts outside accommodation cleaned and PMS change request generated.","2021-04-18T23:59:35","","Completed","2021-04-18T23:59:35","No","No","No","Internal"]
[null,null,null,22242,null,"106_30-10-2021 07:39:00","2021-03-30T23:59:35","Observation","Ship Staff","Ship Staff Insp.","All fire extinguishers to be marked with the inventory serial numbers - permanent stencilling to be done in place.","LSA / FFA","Safety / LSA / FFA","Knowledge Based","5.42","Medium","","","All fire extinguishers marked with the inventory serial numbers permanently.","2021-05-18T23:59:35","","Completed","2021-05-15T23:59:35","No","No","No","Internal"]
[null,null,null,18764,null,"106_17/4/2021 4:24:57 AM","2021-04-04T23:59:35","Defect","Ship Staff","Ship Staff Insp.","vessel has noticed, both Life boat battery charger breaker is tripping frequently due to under rated capacity of breaker.","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.29","High","","","New breaker received and renewed.Tripping issue resolved.","2021-11-28T23:59:35","BCIA210150","Completed","2021-11-12T23:59:35","No","No","No","Internal"]
[null,null,null,18765,null,"106_16/4/2021 10:08:06 PM","2021-04-04T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Annemometer unit in CCR not showing the current wind direction and speed and not giving any alarm in case parameter is exceeded.","Miscellaneous","Cargo / Ballast Systems","Equipment Related","5.9","Very High","","","Alarm setting procedure obtained from Makers and Defect rectified. ","2021-08-29T23:59:35","","Completed","2021-08-26T23:59:35","No","No","No","Internal"]
[null,null,null,18772,null,"106_17/4/2021 4:03:05 AM","2021-04-05T23:59:35","Observation","Ship Staff","Ship Staff Insp."," We observed heavy excessive vibration in the Purifier Room I beam. \n\n\n\n","E/R - Pipes/ valves & fittings","Structural Condn. / WT integrity ","Equipment Related","11.5","Medium","","","Excessive vibration in the Purifier Room I beam restricted by taking Preventive measures , additional support was fabricated and installed by hot work . Vibration has been restricted.\n\n","2021-04-28T23:59:35","","Completed","2021-04-08T23:59:35","No","No","No","Internal"]
[null,null,null,18766,null,"106_16/4/2021 9:36:05 PM","2021-04-06T23:59:35","Guarantee Claim","Ship Staff","Ship Staff Insp.","Pressure Gauges in Bosun Store dislodged from base mounting plate.","Deck - Pipe / Fittings","Emgcy. Systems","Equipment Related","6.1","Medium","","","Gauges secured in position using cable tie and copper wire. GC raised.","2021-07-06T23:59:35","GC-057","Completed","2021-05-11T23:59:35","No","No","No","Internal"]
[null,null,null,18767,null,"106_16/4/2021 9:45:15 PM","2021-04-07T23:59:35","Guarantee Claim","Ship Staff","Ship Staff Insp.","FPK and 1P WBT Air Pipe Head Float Ball damaged due to rough weather","Hull & Tanks","Structural Condn. / WT integrity ","External Factors","11.7","High","","","GC raised.","2021-07-07T23:59:35","GC-058","Completed","2021-05-12T23:59:35","No","No","No","Internal"]
[null,null,null,18768,null,"106_16/4/2021 9:51:14 PM","2021-04-11T23:59:35","Guarantee Claim","Ship Staff","Ship Staff Insp.","Defective SCBA Alarm Whistle ","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.43","High","","","Fault finding carried out. GC raised.","2021-07-11T23:59:35","GC-059","Completed","2021-05-09T23:59:35","No","No","No","Internal"]
[null,null,null,21025,null,"106_12/8/2021 6:35:45 PM","2021-04-19T23:59:35","Guarantee Claim","Ship Staff","Ship Staff Insp.","Pressure gauges on VECS Manifold found defective.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.17","Low","","","Spares received and gauges renewed. Working in order","2021-07-19T23:59:35","GC-061","Completed","2021-05-23T23:59:35","No","No","No","Internal"]
[null,null,null,21026,null,"106_12/8/2021 4:59:38 PM","2021-04-26T23:59:35","Guarantee Claim","Ship Staff","Ship Staff Insp.","AE 1 Exh.Gas T/C inlet digital thermo meter Faulty.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Replaced with Spare one Available on board .GC spare received.","2021-07-26T23:59:35","","Completed","2021-06-16T23:59:35","No","No","No","Internal"]
[null,null,null,21000,null,"106_12/8/2021 6:40:01 PM","2021-05-02T23:59:35","Guarantee Claim","Ship Staff","Ship Staff Insp.","Fixed gas detection system H2S sensor span calibration issue","Hull & Tanks","Cargo / Ballast Systems","Equipment Related","5.21","Medium","","","H2S sensor range adjusted as per maker instructions. Sensor calibrated for ZERO and SPAN, working in order.","2021-11-28T23:59:35","GC-062","Completed","2021-11-24T23:59:35","No","No","No","Internal"]
[null,null,null,21027,null,"106_12/8/2021 9:37:50 PM","2021-05-02T23:59:35","Guarantee Claim","Ship Staff","Ship Staff Insp.","AE #3 Alternator non drive bearing temperature sensor faulty","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Temperature sensor troubleshooting as per maker advise carried out found a wire insulation damaged, same repaired and temp sensor working in order.","2021-08-02T23:59:35","GC 063","Completed","2021-05-23T23:59:35","No","No","No","Internal"]
[null,null,null,20999,null,"106_12/8/2021 9:42:50 PM","2021-05-17T23:59:35","Guarantee Claim","Ship Staff","Ship Staff Insp.","EGCS Cooling down issue after normal stoppage","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Follow up with makers in progress. Exhaust dampers inspected and found all in order. Makers advise requested for further investigations.","2021-12-29T23:59:35","GC-064","Completed","2021-11-09T23:59:35","No","No","No","Internal"]
[null,null,null,19664,null,"106_15/6/2021 4:28:32 AM","2021-06-07T23:59:35","Observation","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","The List of Enclosed spaces provided by the vessel was Generic in content and Not Ship Specific.","Documentation","Cert. & Docu.","Human Error","5.16","Very High","","","List of Enclosed spaces prepared onboard mentioning each specific Enclosed space with tank identification. Old Generic list and new prepared List attached as closure.  \n\nThe List is posted on Notice boards at all prominent locations. \n\nAll spaces as listed are marked with Notice – “Enclosed Space – No Entry Without Permit”.","2021-07-07T23:59:35","NA","Completed","2021-06-07T23:59:35","No","No","No","External"]
[null,null,null,19665,null,"106_15/6/2021 4:53:52 AM","2021-06-07T23:59:35","Defect","PSC Insp.","PSC Inspection","Cargo manifestation of \"H2S level \" was\n\nnot posted in notice board for crews to know and be aware. To be posted.","Miscellaneous","MLC Related","Human Error","","","Other","","MSDS of cargo was posted on all Common notice boards along High H2S Warnings and Dangers associated with high H2S Cargoes. Company Guidelines for handling high H2S Cargoes also posted. \n\nSpecific PPM content of H2S in Vapour space (>1000 ppm) was not included in the notices. Same was however briefed to all in Pre-Arrival cargo meeting and Crew well aware of same\n\n\n\nCorrective Actions : \n\nNotice for H2S Content in Vapor space posted prior inspector disembarked and deficiency verified and closed out by the Inspector.\n\n\n\nPreventive Actions : \n\n1. Toxic Gases content in Vapor spaces of the Cargo to be displayed specifically and manifested in quantity in Common areas and Notice boards. \n\n2. Risk assessment which is made for handling High H2S cargoes to include above control measure for continuing the Practice.\n\n3. NC discussed with all crew members onboard and preventive actions acknowledged.","2021-06-08T23:59:35","NA","Completed","2021-06-07T23:59:35","No","No","No","External"]
[null,null,null,21001,null,"106_12/8/2021 9:49:50 PM","2021-06-12T23:59:35","Guarantee Claim","Ship Staff","Ship Staff Insp.","Main Engine NOx sensor no:1 defective","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Vessel replaced NOx sensor with spare, system working satisfactory. GC spare received at bophorous, turkey.","2021-11-28T23:59:35","GC-066","Completed","2021-11-21T23:59:35","No","No","No","Internal"]
[null,null,null,21035,null,"106_12/8/2021 9:46:05 PM","2021-06-12T23:59:35","Guarantee Claim","Ship Staff","Ship Staff Insp.","EGCS SW inlet pressure switch malfunctioning","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Pressure Switch renewed with spare received under GC.","2021-09-12T23:59:35","GC- 065","Completed","2021-08-18T23:59:35","No","No","No","Internal"]
[null,null,null,21515,null,"106_13/10/2021 10:50:43 PM","2021-06-13T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Waste Oil tank Dial type Temperature gauge found to be opaque, glass to be replaced\t","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Transparent glass renewed and glycerine filled. Gauge readings are visible.","2021-07-13T23:59:35","","Completed","2021-06-28T23:59:35","No","No","No","Internal"]
[null,null,null,21516,null,"106_13/10/2021 10:54:48 PM","2021-06-13T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Hazard warning tiger stripes to be painted on frames in ER bottom platform aft side\t","Miscellaneous","Eng. / Strg. Comp.","Knowledge Based","10.29","Medium","","","Hazard warnings painted yellow & black in ER bottom platform","2021-06-28T23:59:35","","Completed","2021-06-19T23:59:35","No","No","No","Internal"]
[null,null,null,21517,null,"106_13/10/2021 11:15:27 PM","2021-06-13T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Watermist system warning poster located at wrong place , need to be relocated in steering gear door entrance\t\t","LSA / FFA","Eng. / Strg. Comp.","Knowledge Based","5.4","High","","","Poster relocated. ","2021-06-28T23:59:35","","Completed","2021-06-16T23:59:35","No","No","No","Internal"]
[null,null,null,21518,null,"106_13/10/2021 6:07:17 PM","2021-06-13T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Emergency escape in ECR/ER workshop is two stage lifting for rescue. One of the deck, pulley is not fixed. Same to be fixed.","Miscellaneous","Eng. / Strg. Comp.","Knowledge Based","10.15","Low","","","Pulley fixed and tested. All emergency escape route pulley checked.","2021-07-13T23:59:35","","Completed","2021-06-26T23:59:35","No","No","No","Internal"]
[null,null,null,21519,null,"106_13/10/2021 6:09:24 PM","2021-06-13T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Drums in EGCS room found to bes secured with ropes. Same to be secured with wire ropes and bulldog gripes","Miscellaneous","Eng. / Strg. Comp.","Inappropriate Procedure","5.11","Low","","","Drums secured with wire ropes.","2021-07-13T23:59:35","","Completed","2021-06-24T23:59:35","No","No","No","Internal"]
[null,null,null,22154,null,"106_12/8/2021 9:47:05 PM","2021-06-13T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Mast Wires are fitted with sheathings. Unable to inspect the wire condition – Sheathing to be removed and wires to be inspected","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.8","Low","","","Mast Wires sheathings removed, thorough inspection carried out.","2021-07-13T23:59:35","","Completed","2021-07-11T23:59:35","No","No","No","Internal"]
[null,null,null,22155,null,"106_12/8/2021 9:48:05 PM","2021-06-13T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","440 V IMO Symbols missing on Emergency Switch Boards","Deck - Machinery,Elect. Mach. & Equip.","Safety / LSA / FFA","Knowledge Based","5.37","Low","","","IMO Symbol for 440 V placed on Emergency Switch Boards","2021-06-28T23:59:35","","Completed","2021-06-15T23:59:35","No","No","No","Internal"]
[null,null,null,22156,null,"106_12/8/2021 9:49:05 PM","2021-06-13T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Pressure gauges for HHCs are dirty and unreadable. In case damaged GC to be raised for same. ","Deck - Machinery","Cargo / Ballast Systems","Equipment Related","8.5","Very High","","","Upon inspection HHC Pressure gauges found damaged, GC raised GC073. New gauge received and replaced.","2021-08-13T23:59:35","","Completed","2021-08-06T23:59:35","No","No","No","Internal"]
[null,null,null,22157,null,"106_12/8/2021 9:50:05 PM","2021-06-13T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Gymnasium to be secured well. Loose weights stow rack to be prepared.","Accommodation","General Appearance","Behaviour Based","4.4","High","","","Gymnasium securedl. Loose weights stow rack fabricated.","2021-06-28T23:59:35","","Completed","2021-06-26T23:59:35","No","No","No","Internal"]
[null,null,null,22158,null,"106_12/8/2021 9:51:05 PM","2021-06-13T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Lifeboat Gripes PVC coating to be removed and wire to be inspected. Refer Safety flash No. 26/2012. ","LSA / FFA","Safety / LSA / FFA","Knowledge Based","11.8","Low","","","Lifeboat Gripes PVC coating removed and wire  inspected.  ","2021-07-03T23:59:35","","Completed","2021-06-16T23:59:35","No","No","No","Internal"]
[null,null,null,22159,null,"106_12/8/2021 9:52:05 PM","2021-06-13T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","All mushroom vents on deck to stencilled permanently. Id plates are fading and same to be polished and marked well.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Knowledge Based","11.7","High","","","All mushroom vents on deck stencilled permanently. Id plates polished and marked well.","2021-07-12T23:59:35","","Completed","2021-07-08T23:59:35","No","No","No","Internal"]
[null,null,null,22160,null,"106_12/8/2021 9:53:05 PM","2021-06-13T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Mooring winches drum hauling direction to be marked permanently.","Deck - Mooring Machinery","Mooring","Knowledge Based","9.19","Low","","","Mooring winches drum hauling direction permanently marked.","2021-07-12T23:59:35","","Completed","2021-07-01T23:59:35","No","No","No","Internal"]
[null,null,null,21002,null,"106_12/8/2021 9:56:23 PM","2021-06-14T23:59:35","Guarantee Claim","Ship Staff","Ship Staff Insp.","Fire extinguisher3 nos hose found cracked\t","LSA / FFA","Eng. / Strg. Comp.","Equipment Related","5.42","Medium","","","GC raised and awaiting for spare","2021-12-29T23:59:35","GC-067","Completed","2021-11-09T23:59:35","No","No","No","Internal"]
[null,null,null,21036,null,"106_13/8/2021 10:08:44 PM","2021-06-15T23:59:35","Defect,Guarantee Claim","Ship Staff","Ship Staff Insp.","Main Air comp. no.2 OCR faulty and malfuctioning.","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","OCR replaced with re-conditioned spare ,Spare received under GC kept as stby spare.","2021-09-15T23:59:35","GC-069","Completed","2021-08-04T23:59:35","No","No","No","Internal"]
[null,null,null,21003,null,"106_13/8/2021 10:16:40 PM","2021-06-19T23:59:35","Guarantee Claim,Observation","Ship Staff","Ship Staff Insp.","A/E Cylinder HT cooling water presuure gauge showing over range .","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","GC raised and troubleshooting carried out for presure reducing valve. Follow up with yard in progress.","2021-12-29T23:59:35","GC-071","Completed","2021-11-09T23:59:35","No","No","No","Internal"]
[null,null,null,21028,null,"106_13/8/2021 10:12:58 PM","2021-06-19T23:59:35","Defect,Guarantee Claim","Ship Staff","Ship Staff Insp.","Bridge Chart table light dimmer defective","Elect. Mach. & Equip.,Navigation - Others","Navigation","Equipment Related","11.16","Low","","","Dimmer replaced with spare received under GC. Chart table lamp working in order.","2021-09-19T23:59:35","GC-070","Completed","2021-08-14T23:59:35","No","No","No","Internal"]
[null,null,null,21029,null,"106_13/8/2021 10:04:10 PM","2021-06-20T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Officer's laundry washing machine not operational due to faulty drain pump and water drain switch","Accommodation","General Appearance","Equipment Related","11.13","Low","","","Washing machine drain pump and water pressure switch renewed. Working in order.","2021-09-20T23:59:35","GC 068","Completed","2021-08-12T23:59:35","No","No","No","Internal"]
[null,null,null,21030,null,"106_14/8/2021 9:03:30 PM","2021-06-21T23:59:35","Defect,Guarantee Claim","Ship Staff","Ship Staff Insp.","Port lifeboat winch handle interlock limit switch operational issue","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.28","Very High","","","Limit switch renewed with spare received under GC. Limit switch function tested found working in order.","2021-09-21T23:59:35","GC 072","Completed","2021-08-10T23:59:35","No","No","No","Internal"]
[null,null,null,21031,null,"106_14/8/2021 9:08:10 PM","2021-06-21T23:59:35","Defect,Guarantee Claim","Ship Staff","Ship Staff Insp.","Hose handling crane filter indicator damaged.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.5","Very High","","","Filter indicator renewed for hose handling crane after receiving spares under GC","2021-09-21T23:59:35","GC- 073","Completed","2021-08-08T23:59:35","No","No","No","Internal"]
[null,null,null,21004,null,"106_14/8/2021 9:19:32 PM","2021-06-23T23:59:35","Guarantee Claim","Ship Staff","Ship Staff Insp.","STBD Provision crane hoist up limit switch opertional issue\t","Deck - Machinery","Cargo / Ballast Systems","Equipment Related","10.28","Low","","","GC raised and follow up with makers in progress.","2021-12-29T23:59:35","GC 075","Completed","2021-11-09T23:59:35","No","No","No","Internal"]
[null,null,null,21032,null,"106_14/8/2021 9:12:37 PM","2021-06-23T23:59:35","Guarantee Claim","Ship Staff","Ship Staff Insp.","Sound powered telephone(IS) headset found defective","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.41","Medium","","","GC spare received and headset renewed and working satisfactory.","2021-09-23T23:59:35","GC-074","Completed","2021-08-08T23:59:35","No","No","No","Internal"]
[null,null,null,21005,null,"106_14/8/2021 9:22:10 PM","2021-06-29T23:59:35","Defect,Guarantee Claim","Ship Staff","Ship Staff Insp.","VECS oxygen sensor defective","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.17","Low","","","New sensor received and same replaced, system working in order.","2021-11-28T23:59:35","GC 076","Completed","2021-11-24T23:59:35","No","No","No","Internal"]
[null,null,null,21033,null,"106_14/8/2021 9:25:46 PM","2021-07-07T23:59:35","Defect,Guarantee Claim","Ship Staff","Ship Staff Insp.","Fixed gas detection system solenoid valve for AHU air intake defective","Deck - Machinery,Miscellaneous","Cargo / Ballast Systems","Equipment Related","8.46","Very High","","","Solenoid valve renewed with spare onboard. GC spare received, kept as standby spare","2021-10-07T23:59:35","GC 077","Completed","2021-08-05T23:59:35","No","No","No","Internal"]
[null,null,null,21006,null,"106_14/8/2021 9:28:55 PM","2021-07-19T23:59:35","Guarantee Claim,Observation","Ship Staff","Ship Staff Insp.","Clinometer LED light found not operational.\t","Elect. Mach. & Equip.","Navigation","Equipment Related","11.16","Low","","","Troubleshooting carried out and GC raised. Awaiting reply from yard/makers for further troubleshooting.","2021-12-29T23:59:35","GC 078","Completed","2021-11-09T23:59:35","No","No","No","Internal"]
[null,null,null,21007,null,"106_14/8/2021 9:36:53 PM","2021-07-19T23:59:35","Guarantee Claim,Observation","Ship Staff","Ship Staff Insp.","Excessive vibration noticed in ER workshop grinder","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","GC raised and follow up with yard in progress. all foundation bolts tightened and observed to have vibration. Additional support fabricated and fitted. Vibration reduced to a considerable limit. ","2021-12-29T23:59:35","GC 080","Completed","2021-11-09T23:59:35","No","No","No","Internal"]
[null,null,null,21008,null,"106_14/8/2021 9:34:45 PM","2021-07-20T23:59:35","Defect,Guarantee Claim","Ship Staff","Ship Staff Insp.","Fresh Water Generator SW pipeline thermometer pocket and thermometer damage\t","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","FW pipe renewed with spare received. Leak rectified. ","2021-10-20T23:59:35","GC 079","Completed","2021-10-15T23:59:35","No","No","No","Internal"]
[null,null,null,21009,null,"106_14/8/2021 9:41:19 PM","2021-07-21T23:59:35","Guarantee Claim,Observation","Ship Staff","Ship Staff Insp.","Defective light switches in accomodation\t","Accommodation","General Appearance","Equipment Related","11.16","Low","","","Spare switched received and defective ones replaced.","2021-10-18T23:59:35","GC 081","Completed","2021-10-14T23:59:35","No","No","No","Internal"]
[null,null,null,21017,null,"106_14/8/2021 9:47:54 PM","2021-07-24T23:59:35","Guarantee Claim,Observation","Ship Staff","Ship Staff Insp.","Aux boiler No:2 Soot blower not operational","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","PLC for soot blower received and soot blower tried out. Working in order.","2021-11-28T23:59:35","GC 082","Completed","2021-11-22T23:59:35","No","No","No","Internal"]
[null,null,null,21018,null,"106_14/8/2021 11:19:10 PM","2021-07-24T23:59:35","Guarantee Claim,Observation","Ship Staff","Ship Staff Insp.","ME SCR system venting air leakage observed.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","GC raised. Troubleshooting as per makers advise carried out. Received orifice plate for the venting air line, same fitted and still issue persist.Further follow up with makers in progress","2021-12-29T23:59:35","GC 085","Completed","2021-11-09T23:59:35","No","No","No","Internal"]
[null,null,null,22243,null,"106_30-10-2021 07:47:01","2021-07-24T23:59:35","Observation","Ship Staff","Cargo Audit","26-July-2021: loading at Angr Dos Reis, Brazil. Company checklist 12.20.05.291.01 (Ship-Shore Agreement) was not put in use. Personal checklist used instead.","Documentation","Cert. & Docu.","Knowledge Based","","","",""," Vessel will continue to use this checklist in lieu of 12.20.05.291.01 as the checklist in use is provided from the Time charterers and since the same is a commercial document as well","2021-10-23T23:59:35","","Completed","2021-07-30T23:59:35","No","No","No","Internal"]
[null,null,null,22244,null,"106_30-10-2021 07:50:53","2021-07-24T23:59:35","Observation","Ship Staff","Cargo Audit","10-July-2021 Discharging at Tramandai, Brazil. Company checklist 12.20.05.291.01 (Ship-Shore Agreement) was not put in use.personal checklist used instead.","Documentation","Cert. & Docu.","Knowledge Based","","","","","Vessel will continue to use this checklist in lieu of 12.20.05.291.02 as the checklist in use is provided from the time charterer's and since this same is a commercial document as well.","2021-10-23T23:59:35","","Completed","2021-07-30T23:59:35","No","No","No","Internal"]
[null,null,null,22245,null,"106_30-10-2021 07:55:16","2021-07-24T23:59:35","Observation","Ship Staff","Bunkering Audit","18-June-2021 Bunkering at Corpus. In bunker safety checklist the unit of pumping rate mentioned is m3 but, in the bunker plan under \"prior to bunkering checklist, the unit of pumping rate was declared in MT.\" ","Documentation","Cert. & Docu.","Knowledge Based","","","","","Wrongly filled area corrected immediatly i.e in all places transfer rate unit corrected to same unit as m3/hr","2021-10-23T23:59:35","","Completed","2021-07-30T23:59:35","No","No","No","Internal"]
[null,null,null,21010,null,"106_14/8/2021 9:53:23 PM","2021-07-25T23:59:35","Guarantee Claim,Observation","Ship Staff","Ship Staff Insp.","Defective fire door closer in accomodation  & engine room\t","Accommodation","General Appearance","Equipment Related","5.35","Medium","","","Defective fire door closure rectified, communicated with manufacturer.GC closed.","2021-11-28T23:59:35","GC 083","Completed","2021-08-18T23:59:35","No","No","No","Internal"]
[null,null,null,21011,null,"106_14/8/2021 11:16:41 PM","2021-07-25T23:59:35","Guarantee Claim","Ship Staff","Ship Staff Insp.","Cabin shower mixer with thermostatic controller found leaking","Accommodation","General Appearance","Equipment Related","11.13","Low","","","Spare received and defective shower mixer renewed.","2021-10-25T23:59:35","GC 084","Completed","2021-10-13T23:59:35","No","No","No","Internal"]
[null,null,null,21012,null,"106_14/8/2021 11:21:05 PM","2021-07-25T23:59:35","Guarantee Claim,Observation","Ship Staff","Ship Staff Insp.","Grey water tank magnetic level gauge showing level in reverse direction.","Hull & Tanks","Eng. / Strg. Comp.","Equipment Related","10.25","Very High","","","Tank level markings with new graduations received and same fixed. GC closed","2021-10-25T23:59:35","GC 086","Completed","2021-10-17T23:59:35","No","No","No","Internal"]
[null,null,null,21013,null,"106_14/8/2021 11:26:31 PM","2021-07-25T23:59:35","Defect,Guarantee Claim","Ship Staff","Ship Staff Insp.","Master's cabin air con lever control defective","Accommodation","General Appearance","Equipment Related","11.16","Low","","","GC raised and awaiting reply from yard","2021-12-29T23:59:35","GC 087","Completed","2021-11-09T23:59:35","No","No","No","Internal"]
[null,null,null,21014,null,"106_14/8/2021 11:28:31 PM","2021-07-27T23:59:35","Defect,Guarantee Claim","Ship Staff","Ship Staff Insp.","Galley cold cabinet LED light not working","Accommodation,Elect. Mach. & Equip.","General Appearance","Equipment Related","11.13","Low","","","LED light renewed with GC spare. Working satisfactory","2021-11-27T23:59:35","GC 088","Completed","2021-11-24T23:59:35","No","No","No","Internal"]
[null,null,null,21015,null,"106_14/8/2021 11:31:10 PM","2021-07-27T23:59:35","Defect,Guarantee Claim","Ship Staff","Ship Staff Insp.","BWTS sewge pump temp sensor &  Filter no:1 pressure sensor showing offline","Deck - Machinery","Cargo / Ballast Systems","Equipment Related","10.32","Very High","","","Sensors renewed and found working in order.","2021-10-27T23:59:35","GC 089","Completed","2021-10-21T23:59:35","No","No","No","Internal"]
[null,null,null,21016,null,"106_14/8/2021 11:35:03 PM","2021-07-27T23:59:35","Defect,Guarantee Claim","Ship Staff","Ship Staff Insp.","Aux boiler #2 smoke density meter calibration issue","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Smoke density meter Rx card received and changed. Smoke density meter working in order","2021-10-27T23:59:35","Gc 090","Completed","2021-10-14T23:59:35","No","No","No","Internal"]
[null,null,null,21019,null,"106_14/8/2021 11:38:14 PM","2021-07-27T23:59:35","Guarantee Claim,Observation","Ship Staff","Ship Staff Insp.","Aux boiler water level gauge with LED lights issue","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","LED lights in water level gauge are getting fused, GC raised for new LED light fittings, communication with yard in progress","2021-12-29T23:59:35","GC 091","Completed","2021-11-09T23:59:35","No","No","No","Internal"]
[null,null,null,21020,null,"106_14/8/2021 11:40:06 PM","2021-07-27T23:59:35","Defect,Guarantee Claim","Ship Staff","Ship Staff Insp.","Ballast pump running hour meter found not working","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Running hr meter renewed for both ballast pumps","2021-10-27T23:59:35","GC 092","Completed","2021-10-19T23:59:35","No","No","No","Internal"]
[null,null,null,21021,null,"106_14/8/2021 11:42:09 PM","2021-07-27T23:59:35","Defect,Guarantee Claim","Ship Staff","Ship Staff Insp.","Hot water circulating pump mechanical seal found leaking","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","pump overhauled and mechanical seal renewed with onboard spare. GC raised, spare mechanical received and kept as spare","2021-10-27T23:59:35","GC 093","Completed","2021-10-13T23:59:35","No","No","No","Internal"]
[null,null,null,21022,null,"106_14/8/2021 11:44:51 PM","2021-07-27T23:59:35","Defect,Guarantee Claim","Ship Staff","Ship Staff Insp.","Emergency shutdown link system - Port side electric horn with strobe light found not working","Cargo Mach.","Emgcy. Systems","Equipment Related","8.1","Very High","","","New horn received under GC, Working in order.","2021-10-27T23:59:35","GC 094","Completed","2021-10-21T23:59:35","No","No","No","Internal"]
[null,null,null,22246,null,"106_30-10-2021 07:59:04","2021-08-03T23:59:35","Observation","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","Garbage container were built in plastic (combustible) material.","Miscellaneous","MARPOL Related","Equipment Related","6.2","High","","","Waste receptacle bins certificates provided by manufacturers. Same are fiber built and off fire retardant material.","2021-08-28T23:59:35","","Completed","2021-08-13T23:59:35","No","No","No","External"]
[null,null,null,22247,null,"106_31/10/2021 12:35:38 AM","2021-08-03T23:59:35","Observation","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","The initial lifting appliances inspection and certificate for all cranes on board, was dated on 30 July 2020. The limit time frame of 12 months to renew the certificate, as per ILO 152, had been passed.","Cargo Mach.,Documentation","Cert. & Docu.","Industry Issue","8.5","Very High","","","Class Survey which was planned after discharge at ALgeciras carried out in Gibraltar on 07 Aug 2021. Certificate issued.","2021-08-08T23:59:35","","Completed","2021-08-05T23:59:35","No","No","No","External"]
[null,null,null,21023,null,"106_19/8/2021 5:07:02 PM","2021-08-12T23:59:35","Other","Ship Staff","Ship Staff Insp.","Engineering Campaign 03 of 2021: Heating, Ventilation & Air Conditioning","Miscellaneous","Eng. / Strg. Comp.","Knowledge Based","","","","","Campaign completed, CRF sent to office. Will be closed once CRF is amended in PAL.Job created as per CRF","2021-10-12T23:59:35","","Completed","2021-09-08T23:59:35","No","No","No","Internal"]
[null,null,null,22248,null,"106_30-10-2021 08:00:36","2021-08-22T23:59:35","Observation","Ship Staff","Ship Staff Insp.","MOB marker line to be renewed.","LSA / FFA","Safety / LSA / FFA","Behaviour Based","5.31","High","","","MOB marker lines renewed.","2021-08-29T23:59:35","","Completed","2021-08-26T23:59:35","No","No","No","Internal"]
[null,null,null,22249,null,"106_30-10-2021 08:02:39","2021-08-22T23:59:35","Observation","Ship Staff","Ship Staff Insp.","MOB marker Lifebuoys weight to be istencilled near to buoy.","LSA / FFA","Safety / LSA / FFA","Human Error","5.31","High","","","MOB marker Lifebuoys weight istencilled near to buoy.","2021-09-13T23:59:35","","Completed","2021-09-02T23:59:35","No","No","No","Internal"]
[null,null,null,22250,null,"106_30-10-2021 08:04:07","2021-08-22T23:59:35","Observation","Ship Staff","Ship Staff Insp.","fwd liferaft lowering ship side chains to be freed up.","LSA / FFA","Safety / LSA / FFA","Human Error","11.1","High","","","fwd liferaft lowering ship side chains freed up.","2021-09-01T23:59:35","","Completed","2021-09-01T23:59:35","No","No","No","Internal"]
[null,null,null,21034,null,"106_19/9/2021 2:56:27 PM","2021-09-09T23:59:35","Observation","Ship Staff","Ship Staff Insp.","During preparations for lowering Starboard lifeboat it was observed that forward most grab line may get entangled with forward most davit fender.","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.28","Very High","","","The Grab line was shortened out by using a Bull Dog Grip.","2021-09-10T23:59:35","","Completed","2021-09-09T23:59:35","No","No","No","Internal"]
[null,null,null,21024,null,"106_19/9/2021 2:49:35 PM","2021-09-14T23:59:35","Defect","Ship Staff","Ship Staff Insp.","After completion of discharge operations on at Jose Ignacio, ANCAP SBM, Uruguay, it was observed that port side pilot ladder bottom rubber steps damaged due to the impact with tug in moderate sea and swell conditions while embarkation of pilot/Loading Master. ","Deck - Machinery","Safety / LSA / FFA","External Factors","5.47","Medium","","","Received the new Solas approved pilot ladder on 16-Oct-2021 at Sines, Portugal. Same was replaced.","2021-10-05T23:59:35","BCIA210146","Completed","2021-10-14T23:59:35","No","No","No","Internal"]
[null,null,null,22251,null,"106_30-10-2021 08:07:37","2021-09-24T23:59:35","Defect","Ship Staff","Ship Staff Insp.","While closing the drain valve of fireline the spindle broke down along with the operating wheel.","LSA / FFA","Safety / LSA / FFA","Equipment Related","11.4","Very High","","","Broken spindle and wheel fabricated and replaced.","2021-10-06T23:59:35","","Completed","2021-10-01T23:59:35","No","No","No","Internal"]
[null,null,null,21520,null,"106_13/10/2021 6:16:24 PM","2021-09-28T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Ship Staff Insp.","FWG SW outlet pipe pin hole to be rectified. Temporary repair carried out to arrest leak.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Pipe section removed and Pin hole rectified with hot work. Pipe internal coated with Epoxy and tried out. FWG and pipelines are in good order","2021-10-28T23:59:35","","Completed","2021-10-03T23:59:35","No","No","No","Internal"]
[null,null,null,23018,null,"106_16/11/2021 9:42:48 AM","2021-10-03T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","It was observed that Slop starboard cargo tank temperature indication on digital and analogue indicator found to be showing error message and showing erratic reading.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","Temperature sensor received under PO. Same renewed and slop (s) temperature readings found to be normal. ","2022-01-02T23:59:35","BCIA210158 - COT SLOP(S) TEMPERATURE SENSOR","Completed","2021-11-23T23:59:35","No","No","No","Internal"]
[null,null,null,21521,null,"106_13/10/2021 6:13:01 PM","2021-10-04T23:59:35","Defect","Ship Staff","Ship Staff Insp.","ME HPS #1 accumulator oil leak observed during loaded passage. Same to be overhauled at first opportunity","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Due to bad weather overhaul carried out after vessel anchored in discharge port. Accumulator overhauled and diaphragm membrane renewed. Engine tried out after overhaul, found all in order.","2021-10-28T23:59:35","","Completed","2021-10-06T23:59:35","No","No","No","Internal"]
[null,null,null,22252,null,"106_30-10-2021 08:09:55","2021-10-04T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Pumproom evacuation arrangement hooks to be cover with sail twin for protecting from metal to metal contact.","LSA / FFA","Safety / LSA / FFA","Knowledge Based","5.2","Very High","","","Pumproom evacuation arrangement hooks covered with sail twin for protecting from metal to metal contact.","2021-10-28T23:59:35","","Completed","2021-10-06T23:59:35","No","No","No","Internal"]
[null,null,null,22238,null,"106_30-10-2021 06:20:46","2021-10-08T23:59:35","Observation","Owner / Marine / Tech. Suptd.","ISM Audit","Calibration gas not available onboard for H2 sensors in BWTS system","Deck - Machinery","Cargo / Ballast Systems","Equipment Related,Knowledge Based","2.13","Low","","","Calibration gas received and H2 sensor calibrated zero and span","2021-11-28T23:59:35","BCIA210051","Completed","2021-11-11T23:59:35","No","No","No","Internal"]
[null,null,null,22253,null,"106_30-10-2021 06:23:37","2021-10-08T23:59:35","Observation","Owner / Marine / Tech. Suptd.","ISM Audit","Fuel Change over procedure and Critical spare part list latest review by suptd not available during the inspection","Miscellaneous","Eng. / Strg. Comp.","Inappropriate Procedure","10.13","Very High","","","Critical spare part list and Fuel change over procedure sent for office approval and same received. Updated version posted in respective locations.","2021-11-28T23:59:35","","Completed","2021-10-21T23:59:35","No","No","No","Internal"]
[null,null,null,22254,null,"106_30-10-2021 06:14:04","2021-10-08T23:59:35","Non Conformity","Owner / Marine / Tech. Suptd.","ISM Audit","ER Cofferdam around void spaces to be inspected every 6 months. Last inspected in Sept2020. No PMS job exist in PAL. ","Hull & Tanks","Eng. / Strg. Comp.","Inappropriate Procedure","2.9","Medium","","","PMS change request sent for office approval and job order added. Tank inspection carried out and Job updated in PAL PMS with inspection report.","2021-11-28T23:59:35","","Completed","2021-10-14T23:59:35","No","No","No","Internal"]
[null,null,null,22255,null,"106_30-10-2021 06:29:58","2021-10-08T23:59:35","Observation","Owner / Marine / Tech. Suptd.","ISM Audit","Unitor chemical Fore & Aft marked alkaline, but kept in the neutral section. Chemical locker to be arranged as per chemical property.","Miscellaneous","Eng. / Strg. Comp.","Human Error,Knowledge Based","5.46","Medium","","","All chemical locker racks checked and arranged as per the pH value. A list of chemicals and its grade highlighted posted in the chemical locker for easy reference","2021-11-28T23:59:35","","Completed","2021-10-17T23:59:35","No","No","No","Internal"]
[null,null,null,22256,null,"106_30-10-2021 06:34:58","2021-10-08T23:59:35","Observation","Owner / Marine / Tech. Suptd.","ISM Audit","SMS checklist for Emergency Generator, Steering gear,etc entered in logbook but without checklist number. As per Company sms laminated checklist can be used but a logbook entry must be maintained.","Documentation","Cert. & Docu.","Inappropriate Procedure","10.5","Low","","","Logbook entries with relevant checklist number logged and all officers have been instructed to follow company procedures.","2021-11-28T23:59:35","","Completed","2021-10-18T23:59:35","No","No","No","Internal"]
[null,null,null,22257,null,"106_30-10-2021 08:13:31","2021-10-08T23:59:35","Observation","Owner / Marine / Tech. Suptd.","ISM Audit","Risk assessment for carrying inspection of Aft Void space not attached to PMS job V-BCIA009516/21 which is required as per the job sepcification. Risk assessment for same sighted in vessel's record.","Documentation","Cert. & Docu.","Knowledge Based","","","","","Ra attached in the job order during internal audit inspection.","2021-12-29T23:59:35","","Completed","2021-10-17T23:59:35","No","No","No","Internal"]
[null,null,null,22258,null,"106_30-10-2021 08:16:02","2021-10-08T23:59:35","Observation","Owner / Marine / Tech. Suptd.","ISM Audit","No PMS job for cargo tank IG valves maintenance and integrity checks. No maintenance record found for same.","Inert Gas","Cargo / Ballast Systems","Knowledge Based","8.23","Medium","","","PMs job created and introduced in PAL.Job carried out as per the job description and reported in PMS.","2021-12-29T23:59:35","","Completed","2021-10-14T23:59:35","No","No","No","Internal"]
[null,null,null,22259,null,"106_30-10-2021 08:18:17","2021-10-08T23:59:35","Observation","Owner / Marine / Tech. Suptd.","ISM Audit","Sopep inventory not updated since last two months in the Sopep plan and also in the Sopep store.Last update sighted 01-Aug-2021.","Documentation","MARPOL Related","Knowledge Based","","","","","Sopep inventory updated for October month in sopep plan as well as in the sopep store immediatly during inspection.","2021-12-28T23:59:35","","Completed","2021-10-14T23:59:35","No","No","No","Internal"]
[null,null,null,22260,null,"106_30-10-2021 08:20:42","2021-10-08T23:59:35","Observation","Owner / Marine / Tech. Suptd.","ISM Audit","Cargo tanks, Ballast tanks and Void spaces are restricted areas as per SSP section 6.02. However same not marked at the enterance of the spaces.","Hull & Tanks","ISPS Related","Knowledge Based","7.1","High","","","Enterance of the cargo tanks, ballast tanks and void spaces were marked with \"Restricted areas - No unauthorised entry\" as per SSP section 6.02.","2021-12-29T23:59:35","","Completed","2021-10-15T23:59:35","No","No","No","Internal"]
[null,null,null,22263,null,"106_30-10-2021 06:26:08","2021-10-08T23:59:35","Observation","Owner / Marine / Tech. Suptd.","ISM Audit","No calibration record available for ER pressure and temperature gauges.","E/R - Aux. Engine,E/R - Aux. Mach.,E/R - Boiler,E/R - Main Engine","Eng. / Strg. Comp.","Inappropriate Procedure,Knowledge Based","8.13","Medium","","","Calibration of Pressure and temperature gauges record updated and maintained. ","2021-11-28T23:59:35","","Completed","2021-10-21T23:59:35","No","No","No","Internal"]
[null,null,null,22261,null,"106_30-10-2021 06:37:33","2021-10-09T23:59:35","Observation","Ship Staff","Ship Staff Insp.","EGCS SW pump no:1 suction line found to have minor pin hole leak. Same to be rectified at the earliest","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Suction pipe section dismantled and hotwork carried out in ER workshop. Leak rectified and assembled in place. Pump tried out found all in order and no leaks.","2021-11-09T23:59:35","","Completed","2021-10-10T23:59:35","No","No","No","Internal"]
[null,null,null,22262,null,"106_30-10-2021 06:41:09","2021-10-21T23:59:35","Defect","Ship Staff","Ship Staff Insp.","ME Lube oil Purifier no:1 fault alarm received upon investigation found belt for the purifier had worn out and broken. Same to be overhauled and belt replaced.","E/R - Purifier","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Belt replaced , bowl cleaning carried out as per maker manual. Purifier tried out and working in order.","2021-11-13T23:59:35","","Completed","2021-10-23T23:59:35","No","No","No","Internal"]
[null,null,null,19661,null,"106_15/6/2021 4:08:49 AM","2021-10-27T23:59:35","Non Conformity","Ship Staff","Ship Staff Insp.","Working Life-jackets onboard not in compliance with the requirements of LSA Code 2.2.1.5 - The method of securing the lifejackets involves securing of knots - Not in line with the requirement.","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.32","High","","","NCN Raised - BCIA/ODEF/2021/S5. Office Notified and acknowledgement received. To be supplied in bulk to all ships.New LSA compliance life jackets received ","2022-01-13T23:59:35","Office Bulk PO","Completed","2022-01-05T23:59:35","No","No","No","Internal","RO will be supplied during vsl call at Singapore"]
[null,null,null,23019,null,"106_16/11/2021 4:13:23 PM","2021-11-07T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Cargo tank heating return line found isolated with a blank, same was not marked and when tried heating steam return was not flowing to cscade tank","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.15","High","","","return pipe section one by one checked for blokage and found the blank in one section in engine room return line. Same removed and heating of tanks carried out after tightening the flanges","2021-11-08T23:59:35","","Completed","2021-11-08T23:59:35","No","No","No","Internal"]
[null,null,null,23020,null,"106_16/11/2021 9:52:53 AM","2021-11-07T23:59:35","Defect","Ship Staff","Ship Staff Insp.","During cargo operation one of the steam line drian valve wheel broke down.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.15","High","","","valve spindle repair carried out and valve made operational. ","2021-11-28T23:59:35","","Completed","2021-11-14T23:59:35","No","No","No","Internal"]
[null,null,null,23021,null,"106_1/12/2021 4:27:09 PM","2021-11-25T23:59:35","Defect","Ship Staff","Ship Staff Insp.","AE EGCS scrubber tripping on high level. Upon investigation found outlet pipe rubber coating found bulged and restricting water flow from scrubbers. Same to be repaired.","E/R - Aux. Mach.,E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Pipe disconnected and rubber coating removed. Pipe internals coated with epoxy paint and assembled back. AE scrubber operating in good order.","2021-11-28T23:59:35","","Completed","2021-11-25T23:59:35","No","No","No","Internal"]
[null,null,null,23339,null,"106_16/12/2021 2:32:57 PM","2021-12-05T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Aux Engine EGCS flowmeter defective. less flow is measured","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.11","Medium","","","Flowmeter renewed with new spare received at cape town on 16th feb 2022","2022-02-26T23:59:35","BCIA210187","Completed","2022-02-25T23:59:35","No","No","No","Internal","RO will be supplied once ready at next convenient port."]
[null,null,null,23340,null,"106_4/1/2022 5:32:05 AM","2021-12-23T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Main SCR PC UPS defective","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.37","Medium","","","Supply to PC is directly given bypassing the UPS.new ups received at singapore and faulty one renewed","2022-01-13T23:59:35","BCIA220019","Completed","2022-01-05T23:59:35","No","No","No","Internal","RO will be supplied during vsl call at Singapore"]
[null,null,null,23654,null,"106_17/1/2022 8:34:59 PM","2022-01-05T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ER Ventilation damper pneumatic actuator protective cover damage, to be renew.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","New protective cover plate fabricated and fitted","2022-02-05T23:59:35","","Completed","2022-03-25T23:59:35","No","No","No","Internal","Noted, please keep update."]
[null,null,null,23655,null,"106_17/1/2022 8:43:34 PM","2022-01-05T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Final coating partially detached on top side of Stbd side hull shall plate IWO No.2 WBT. Re-coating is required.","Hull & Tanks","General Appearance","Equipment Related","2.15","Low","","","Thorough rinsing with Fresh water carried out. Touch up coat applied after mild buffing.","2022-02-05T23:59:35","","Completed","2022-01-22T23:59:35","No","No","No","Internal","Noted, please get permission from office prior to commence the job."]
[null,null,null,23656,null,"106_17/1/2022 9:36:27 PM","2022-01-05T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","One pc of spare IG pipe for Ballast Tank was kept on main deck, exposed to weather.","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.4","Very High","","","Spool piece well greased and covered with canvas.","2022-01-25T23:59:35","","Completed","2022-01-14T23:59:35","No","No","No","Internal","please update once job completed."]
[null,null,null,23657,null,"106_17/1/2022 9:45:25 PM","2022-01-05T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Main engine new spare piston ring was kept in ER 3rd deck without properly packed","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","piston rings  wrapped with plastic after appliying grease","2022-02-05T23:59:35","","Completed","2022-01-25T23:59:35","No","No","No","Internal","please update once job completed."]
[null,null,null,23658,null,"106_17/1/2022 9:51:16 PM","2022-01-05T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Main Engine SCR Sealing air was reported to be higher consumption, maker’s service engineer being consulted","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Vessel carried out the leak test and fault located with leaking service air compressor safety valve.same renewed with spare.and excess leakage issue rectified","2022-03-05T23:59:35","","Completed","2022-01-24T23:59:35","No","No","No","Internal","please keep monitoring and update."]
[null,null,null,23659,null,"106_17/1/2022 8:39:45 PM","2022-01-05T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Paint partially detached on top side of Port side hull shell plate IWO No.5 WBT, rust development observed. De-rusting and coating to be attended.","Hull & Tanks","General Appearance","Equipment Related","2.15","Low","","","Derusting and buffing with pneumatic tools carried out. Rinsing with fresh water done. 1 coat primer and final coat applied.","2022-02-05T23:59:35","","Completed","2022-01-22T23:59:35","No","No","No","Internal","please get permission form office once job completed."]
[null,null,null,23660,null,"106_17/1/2022 8:58:59 PM","2022-01-05T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Fire door between officer mess room and galley is kept at open position during inspection","Accommodation","Safety / LSA / FFA","Inappropriate Procedure","5.35","Medium","","","fire door kept closed and warning notice posted, KEEP KEPT CLOSED ALL TIMES","2022-01-05T23:59:35","","Completed","2022-01-05T23:59:35","No","No","No","Internal"]
[null,null,null,23661,null,"106_17/1/2022 9:14:29 PM","2022-01-05T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","No eye washer available in PPE box in battery room","Miscellaneous","Safety / LSA / FFA","External Factors","5.46","Medium","","","Expired eye wash taken out while at singapore to landing ashore, Same replenished once received","2022-01-12T23:59:35","","Completed","2022-01-05T23:59:35","No","No","No","Internal"]
[null,null,null,23662,null,"106_17/1/2022 9:22:25 PM","2022-01-05T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Sample bottle in sample box was not kept in order","Miscellaneous","General Appearance","Behaviour Based","","","","","Sample bottle rearranged and MSDS verified","2022-01-20T23:59:35","","Completed","2022-01-12T23:59:35","No","No","No","Internal"]
[null,null,null,23663,null,"106_17/1/2022 10:14:37 PM","2022-01-05T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Pressure gauge on Deck steam return observation tank defect, to be renewed.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","11.4","Very High","","","Steam return observation tank has temperature gauge fitted, same found working in order. ","2022-01-29T23:59:35","","Completed","2022-01-14T23:59:35","No","No","No","Internal"]
[null,null,null,23664,null,"106_17/1/2022 8:51:29 PM","2022-01-05T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Smoke room door self closing device not working properly","Accommodation","Safety / LSA / FFA","Equipment Related","5.35","Medium","","","Door closer adjusted and door closing properly.","2022-01-25T23:59:35","","Completed","2022-01-10T23:59:35","No","No","No","Internal"]
[null,null,null,23665,null,"106_17/1/2022 9:29:12 PM","2022-01-05T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Deck steam return observation tank top cover bolt and nut slightly rusted. De-rusting and coating to be attended.","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.4","Very High","","","Derusting of observation tank and fresh coat of paint applied. ","2022-02-05T23:59:35","","Completed","2022-01-12T23:59:35","No","No","No","Internal"]
[null,null,null,23666,null,"106_17/1/2022 9:41:01 PM","2022-01-05T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Deck fire line drain valve in front of accommodation slightly rusted.","Deck - Pipe / Fittings","General Appearance","Equipment Related","11.4","Very High","","","Drain valve derusting carried out and paint applied.","2022-01-25T23:59:35","","Completed","2022-01-13T23:59:35","No","No","No","Internal"]
[null,null,null,23667,null,"106_17/1/2022 9:06:29 PM","2022-01-05T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","There was no mark for air supply valve for air horn","Deck - Pipe / Fittings","General Appearance","Knowledge Based","","","","","Stencil marked air horn supply valve for clear identification","2022-01-20T23:59:35","","Completed","2022-01-11T23:59:35","No","No","No","Internal"]
[null,null,null,24669,null,"106_31/1/2022 7:37:45 AM","2022-01-21T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","Main engine Auxiliary blower #2 motor insulation failed.Motor not operational.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Motor renewed with spare and made operational","2022-01-23T23:59:35","","Completed","2022-01-22T23:59:35","No","No","No","Internal"]
[null,null,null,24670,null,"106_31/1/2022 7:40:58 AM","2022-01-23T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","MAin Engine Auxiliary Blower#2 motor MCCB defective, tripping on motor starting","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Renewed with spare MCCB supplied at Singapore on 28th jan 2022","2022-01-28T23:59:35","","Completed","2022-01-27T23:59:35","No","No","No","Internal"]
[null,null,null,23338,null,"106_16/12/2021 1:18:48 PM","2022-01-28T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Main Engine EGCS gas Sampling pump defective , found piston/diaphram arrangement damaged","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.11","Medium","","","System is working with measured gas value prior breakdown. Ensured full flow of wash water while in operation to attain min so2 to co2 ratio - 9th May 2022 spares received and replaced. System working satisfactory.","2022-04-18T23:59:35","BCIA210187","Completed","2022-05-07T23:59:35","No","No","No","Internal","RO will be supplied once ready at next convenient port."]
[null,null,null,24671,null,"106_15/2/2022 10:01:19 AM","2022-02-10T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Engine room sludge pump failed to take suction.On investigation found the pump stator worned out excessively.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Pump stator renewed with spare.Pump assembled tried out working good.","2022-02-12T23:59:35","","Completed","2022-02-10T23:59:35","No","No","No","Internal"]
[null,null,null,24672,null,"106_31/3/2022 9:52:06 AM","2022-03-17T23:59:35","Critical Equipment","Ship Staff","Ship Staff Insp.","Main Engine NO3 Oil mist detector Fan Fault alarm","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.21","Medium","","","Detector renewed with spare detector onbaord.","2022-03-17T23:59:35","","Completed","2022-03-17T23:59:35","No","No","No","Internal"]
[null,null,null,24974,null,"106_16/4/2022 5:26:46 PM","2022-04-13T23:59:35","Defect","Ship Staff","Ship Staff Insp.","X band radar scanner unit not operational","Navigation - RADAR","Navigation","Equipment Related","4.7","High","","","S band radar scanner switching set for S & X band radar, Shore technician visited at singapore and fault rectified.","2022-04-18T23:59:35","","Completed","2022-04-16T23:59:35","No","No","No","Internal"]
[null,null,null,25307,53472,"106_Mon May 16 2022 21:23:04 GMT+0800","2022-04-17T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Pressure transmitter for Service, control air & SCR air bottle erratic.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Found Pr. transmitter faulty. RO BCIA220043 raised for pressure transmitter. New pressure transmitter fitted. Working satisfactory.","2022-07-30T23:59:35","BCIA220043","Completed","2022-06-21T23:59:35","No","No","No","Internal"]
[null,null,null,25308,17121,"106_Mon May 16 2022 21:27:18 GMT+0800","2022-04-17T23:59:35","Defect,Observation","Ship Staff","Ship Staff Insp.","IG blower area no.2 O2 sensor not working","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","found sensor defective, RO BCIA220036 raised. New O2 sensor fitted. sensor calibrated. working satisfactory.","2022-07-30T23:59:35","BCIA220036","Completed","2022-07-02T23:59:35","No","No","No","Internal"]
[null,null,null,25306,67889,"106_Mon May 09 2022 14:16:33 GMT+0800","2022-05-02T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Mast raiser VOCON automatic valve pressure sensor faulty. ","Inert Gas","Cargo / Ballast Systems","Equipment Related","8.19","High","","","RO raised for new spare sensor. Sensor replaced with spare new one. VOCON valve automatic and manual operation tried out working satisfactory.","2022-06-28T23:59:35","BCIA220092","Completed","2022-08-03T23:59:35","No","No","No","Internal"]
[null,null,null,25304,77135,"106_Mon May 09 2022 11:30:11 GMT+0800","2022-05-07T23:59:35","Observation,Defect","Ship Staff","Ship Staff Insp.","Aux. boiler individual exhaust O2 analyzer HMI panel faulty ","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Fault finding to carry out. Fault finding carried out found sensor faulty.  RO BCIA220104 raised for spare sensors. new senor fitted and calibrated. Working satisfactory.","2022-07-13T23:59:35","BCIA220104","Completed","2022-07-02T23:59:35","No","No","No","Internal"]
[null,null,null,25305,54201,"106_Mon May 09 2022 11:37:57 GMT+0800","2022-05-07T23:59:35","Observation","Ship Staff","Ship Staff Insp.","AE performance measuring device, IMES showing P comp > P  max. ","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Maker consultation under process for calibration of equipment. Maker consultation carried out and the value of Pcomp. equal or slightly greater than Pmax. is normal to our engine design.  Mail forwarded to YANMAR for clarification.","2022-07-13T23:59:35","","Completed","2022-05-25T23:59:35","No","No","No","Internal"]
[null,null,null,25310,35006,"106_Mon May 16 2022 21:34:14 GMT+0800","2022-05-12T23:59:35","Observation,Defect","Ship Staff","Ship Staff Insp.","Calorifier electrical heater showing low insulation.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.3","Medium","","","Fault finding to be carried out. One phase of the heater coil showing low insulation.  Spare heater on board not of same design. RO BCIA220103 raised. New electric heater fitted. Working satisfactory.","2022-07-14T23:59:35","BCIA220103","Completed","2022-06-21T23:59:35","No","No","No","Internal"]
[null,null,null,28491,87329,"0_Mon Jan 16 2023 19:59:55 GMT+0800","2022-05-21T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Electric socket for Wet Garbage freezer in Garbage locker to secure. ","Elect. Mach. & Equip.","General Appearance","Human Error,Behaviour Based,Inappropriate Procedure","11.1","High","","","Electric socket for Wet Garbage freezer in Garbage locker secured. ","2022-06-06T23:59:35","","Completed","2022-05-22T23:59:35","No","No","No","Internal"]
[null,null,null,28492,90382,"0_Mon Jan 16 2023 19:57:25 GMT+0800","2022-05-21T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Mast riser Sprinkler valve to highlight and stencil.","Deck - Pipe / Fittings,Miscellaneous","Safety / LSA / FFA","Inappropriate Procedure,Human Error","5.35","Medium","","","Mast riser Sprinkler valve highlighted and stencilled.","2022-06-06T23:59:35","","Completed","2022-05-25T23:59:35","No","No","No","Internal"]
[null,null,null,28493,17653,"0_Mon Jan 16 2023 20:10:42 GMT+0800","2022-05-21T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Spot rust observed on IG Pipe fittings near Port side accommodation and at Fresh air inlet for AHU. ","Accommodation","General Appearance","Human Error,External Factors","11.4","Very High","","","De-rusting/Painting done on IG Pipe fittings near Port side accommodation and at Fresh air inlet for AHU. ","2022-06-21T23:59:35","","Completed","2022-05-25T23:59:35","No","No","No","Internal"]
[null,null,null,28495,37218,"106_Mon Jan 16 2023 19:50:32 GMT+0800","2022-05-21T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Upper Deck and A Deck toilet floor tiles stains to be cleaned.","Accommodation","General Appearance","Behaviour Based,Human Error","11.13","Low","","","Upper Deck and 'A' deck toilets thoroughly cleaned and stains removed.","2022-06-21T23:59:35","","Completed","2022-05-23T23:59:35","No","No","No","Internal"]
[null,null,null,28498,16015,"0_Mon Jan 16 2023 19:53:38 GMT+0800","2022-05-21T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","All mooring tails and Mooring ropes in use and as spare are not marked and tagged. ","Miscellaneous","Mooring","Behaviour Based,Inappropriate Procedure","9.17","High","","","All mooring tails and Mooring ropes in use and as spare marked and tagged. ","2022-06-21T23:59:35","","Completed","2022-06-29T23:59:35","No","No","No","Internal"]
[null,null,null,28499,38227,"106_Mon Jan 16 2023 19:39:12 GMT+0800","2022-05-21T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Max stowage line for Sprinkler not marked in Port and Stbd midship store.","Miscellaneous","Safety / LSA / FFA","Inappropriate Procedure","5.35","Medium","","","Max Stowage line marked inside Port & stbd Midship store and stencilled.","2022-06-06T23:59:35","","Completed","2022-05-23T23:59:35","No","No","No","Internal"]
[null,null,null,28500,19141,"0_Mon Jan 16 2023 20:15:48 GMT+0800","2022-05-21T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Metal plate of Lifeboat launching instructions on ‘A’ Deck to clean and varnish. ","LSA / FFA","General Appearance","Behaviour Based,External Factors","5.27","Medium","","","Metal plate of Lifeboat launching instructions on ‘A’ Deck cleaned and varnished. ","2022-06-06T23:59:35","","Completed","2022-05-23T23:59:35","No","No","No","Internal"]
[null,null,null,28501,12922,"0_Mon Jan 16 2023 20:27:20 GMT+0800","2022-05-21T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Inlet hose for Portable Foam applicator getting squeezed due to the cover of the box and will develop cracks. To prepare some alternative arrangement to prevent the same. ","LSA / FFA","Safety / LSA / FFA","Behaviour Based,Knowledge Based,Inappropriate Procedure","5.42","Medium","","","Inlet hose for Portable Foam Applicator coiled and kept clear of the cover in order to avoid squeezing/damage.","2022-06-21T23:59:35","","Completed","2022-05-22T23:59:35","No","No","No","Internal"]
[null,null,null,28502,57151,"0_Mon Jan 16 2023 20:31:48 GMT+0800","2022-05-21T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Spot rust and weeping marks observed on Lifeboat Davits (P & S). ","LSA / FFA","Safety / LSA / FFA","Behaviour Based,External Factors","5.28","Very High","","","De-rusting/Painting of spot rust carried out on Port & Stbd Lifeboat davits. Weep marks cleaned.","2022-06-21T23:59:35","","Completed","2022-05-24T23:59:35","No","No","No","Internal"]
[null,null,null,28504,13221,"0_Mon Jan 16 2023 20:07:14 GMT+0800","2022-05-21T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Galley Exhaust mesh on ‘B’ Deck port side to clean of Oil and Grease deposits. ","Miscellaneous","Safety / LSA / FFA","Human Error,Inappropriate Procedure","11.13","Low","","","Galley Exhaust mesh on ‘B’ Deck port side oil deposits and grease cleaned. ","2022-06-06T23:59:35","","Completed","2022-05-23T23:59:35","No","No","No","Internal"]
[null,null,null,25746,63508,"106_Tue May 31 2022 21:47:43 GMT+0800","2022-05-25T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Fire and GS pump suction valve not holding.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Suction valves tried operating manually by removing easing gear, still not holding. RO BCIA220112 raised for valves. Suction valves renewed with spare supplied.","2022-08-28T23:59:35","BCIA220112","Completed","2022-08-10T23:59:35","No","No","No","Internal"]
[null,null,null,25748,33985,"106_Tue May 31 2022 21:56:54 GMT+0800","2022-05-26T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Pump room FGDS O2 sensor showing low O2 alarm","Deck - Machinery","Safety / LSA / FFA","Equipment Related","5.21","Medium","","","Calibration of O2 sensor carried out, Office consultation carried out and procedure followed. RO BCIA220114 raised for spare O2 sensor. New O2 sensor fitted, calibrated. Working satisfactory.","2022-06-18T23:59:35","BCIA220114","Completed","2022-06-20T23:59:35","No","No","No","Internal"]
[null,null,null,25747,12827,"106_Thu Jun 16 2022 18:04:38 GMT+0800","2022-06-11T23:59:35","Defect","Ship Staff","Ship Staff Insp.","CCR Anemometer printer not printing","Miscellaneous","Cargo / Ballast Systems","Equipment Related","11.16","Low","","","Maker consultation carried out,  Fault finding carried out as per maker recommendation. PSU ordered by maker, to renew upon receipt. PSU renewed. Printer working satisfactory.","2022-08-28T23:59:35","","Completed","2022-06-20T23:59:35","No","No","No","Internal"]
[null,null,null,26720,17059,"106_Fri Jul 15 2022 12:06:28 GMT+0800","2022-07-09T23:59:35","Observation","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","No.6 Port COT temperature sensor TM,TL error to rectify. As per SIRE inspector observation.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.13","Medium","","","Maker consultation under process, RO BCIA220155 raised for spare temperature sensor and PCB board. Spare sensor TM,TL received. Upon fault finding noticed after swapping E-box fault got rectified. RO BCIA220171 raised for spare E-box. Received spare E-box , temperature PCB received at caleta cordova, same replaced and re programming carried out. Found working satisfactory  ","2022-12-28T23:59:35","BCIA220171","Completed","2022-10-31T23:59:35","No","No","No","External"]
[null,null,null,28532,60698,"0_Tue Jan 17 2023 19:49:39 GMT+0800","2022-08-13T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Cleaning of Exhaust trunking in Galley.","Accommodation","General Appearance","Behaviour Based,Human Error","11.13","Low","","","Exhaust trunking in Galley cleaned.","2022-08-28T23:59:35","","Completed","2022-08-16T23:59:35","No","No","No","Internal"]
[null,null,null,28533,84487,"0_Tue Jan 17 2023 19:57:08 GMT+0800","2022-08-13T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Paint mark on the gauge glass of aft spring winch to be removed.","Deck - Mooring Machinery","Mooring","External Factors,Human Error,Inappropriate Procedure","9.14","Medium","","","Paint mark on the gauge glass of aft spring winch cleaned.","2022-08-23T23:59:35","","Completed","2022-08-15T23:59:35","No","No","No","Internal"]
[null,null,null,28534,84132,"0_Tue Jan 17 2023 19:53:56 GMT+0800","2022-08-13T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Lose Lagging in the AC room to be covered.","Elect. Mach. & Equip.","General Appearance","Equipment Related,Inappropriate Procedure,Human Error","11.16","Low","","","Lose Lagging in the AC room covered and rectified.","2022-08-28T23:59:35","","Completed","2022-08-21T23:59:35","No","No","No","Internal"]
[null,null,null,28535,85485,"0_Tue Jan 17 2023 19:59:50 GMT+0800","2022-08-13T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Winch Brake Band resting nut clearance of all winches & windlass to be adjusted to 3-5mm","Deck - Mooring Machinery","Mooring","Behaviour Based,Equipment Related,Inappropriate Procedure","9.15","Medium","","","Winch Brake Band resting nut clearance of all winches & windlass checked and adjusted to 3-5mm.","2022-09-13T23:59:35","","Completed","2022-09-06T23:59:35","No","No","No","Internal"]
[null,null,null,28536,92949,"0_Tue Jan 17 2023 20:02:04 GMT+0800","2022-08-13T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","General Cleaning of forepeak store.","Miscellaneous","General Appearance","Human Error,Behaviour Based","11.12","Low","","","Forepeak store cleaned and arranged.","2022-08-23T23:59:35","","Completed","2022-08-17T23:59:35","No","No","No","Internal"]
[null,null,null,28537,69070,"106_Tue Jan 17 2023 19:47:44 GMT+0800","2022-08-13T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","General Cleaning of Messroom.","Accommodation","General Appearance","Behaviour Based,Human Error","11.13","Low","","","Both Crew & Officer's Messroom cleaned.","2022-08-23T23:59:35","","Completed","2022-08-15T23:59:35","No","No","No","Internal"]
[null,null,null,25303,14167,"106_Tue May 17 2022 10:39:34 GMT+0800","2022-08-13T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Separate Stowage arrangement to be fabricated to stow the manifold and misc. gaskets in the midship store in order to avoid getting damaged.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Inappropriate Procedure","5.11","Low","","","Separate Stowage arrangement fabricated to stow the manifold and misc. gaskets in the midship store in order to avoid getting damaged. ","2022-09-13T23:59:35","None","Completed","2022-08-15T23:59:35","No","No","No","Internal"]
[null,null,null,25311,12236,"106_Mon May 16 2022 21:42:46 GMT+0800","2022-08-13T23:59:35","Defect,Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ME LDCL temperature control valve slight leaking from the spindle, during maneuvering.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.3","Medium","","","Temporary repair carried out, no leak in the system. RO will be raised for spare O-rings. RO BCIA220102 raised, Leak rectified.","2022-09-13T23:59:35","BCIA220102","Completed","2022-09-03T23:59:35","No","No","No","Internal"]
[null,null,null,25312,63985,"106_Mon May 16 2022 21:46:15 GMT+0800","2022-08-13T23:59:35","Defect,Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ME SCR nox. sensor showing wrong reading.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.3","Medium","","","Rebooting of system carried out, still fault exist. Nox. sensor renewed with spare one, working satisfactory.","2022-08-23T23:59:35","","Completed","2022-08-21T23:59:35","No","No","No","Internal"]
[null,null,null,25313,82134,"0_Tue May 17 2022 10:49:02 GMT+0800","2022-08-13T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Trelleborg COP Remote trip not used by vessel during discharge operations, same to be used when possible during discharge/STS operations. ","Deck - Machinery","Safety / LSA / FFA","Human Error","8.3","Very High","","","System tested as part of pre arrival cargo operations tests and checks.  System working in good order. Vessel will start using the system from next discharging operation onwards.","2022-08-20T23:59:35","","Completed","2022-08-17T23:59:35","No","No","No","Internal"]
[null,null,null,25314,23092,"0_Tue May 17 2022 10:57:09 GMT+0800","2022-08-13T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Port/stbd Gangway Davit lashing wire found to have 2 wire clips instead of 3","Deck - Machinery","Safety / LSA / FFA","Human Error","5.47","Medium","","","Additional wire clip used. Both port & stbd gangway davit lashing wires constitues 3 wire clips.","2022-08-28T23:59:35","NA","Completed","2022-08-17T23:59:35","No","No","No","Internal"]
[null,null,null,25315,91815,"0_Tue May 17 2022 10:59:15 GMT+0800","2022-08-13T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Spare anchor stowed on main deck area aft of port side manifold is secured with lashing wire and fixed bracket arrangement. Lashing wire is found to have 2 wire clips instead of 3.","Miscellaneous","Safety / LSA / FFA","Human Error","9.2","Very High","","","Additional wire clip used. Spare anchor lashing wire now constitues 3 wire clips.","2022-08-28T23:59:35","","Completed","2022-08-17T23:59:35","No","No","No","Internal"]
[null,null,null,25316,46470,"0_Tue May 17 2022 11:02:32 GMT+0800","2022-08-13T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Stbd. anchor lashing is done using 3 nos. of 12mm diameter wire rope sling instead of 30 mm wire rope sling.","Deck - Machinery","Safety / LSA / FFA","Human Error","9.20","Medium","","","New lashing wires received in SIngapore on 18.April.2022.  Both anchor lashing wire replaced with new ones (30mm wire sling).","2022-08-28T23:59:35","","Completed","2022-08-15T23:59:35","No","No","No","Internal"]
[null,null,null,25317,27899,"0_Tue May 17 2022 11:06:58 GMT+0800","2022-08-13T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","COT 1Ws steam lines observed to have excessive salt depositions. Same to be cleaned and lines to be re- painted.","Deck - Pipe / Fittings","General Appearance","External Factors","11.4","Very High","","","Steam lines derusted and buffed. All salt deposits and ginger rust cleared. Applied 2 coats of high temp paint.","2022-09-13T23:59:35","","Completed","2022-09-06T23:59:35","No","No","No","Internal"]
[null,null,null,27314,88534,"106_Sun Oct 30 2022 04:06:40 GMT+0800","2022-08-31T23:59:35","Observation","Ship Staff","Ship Staff Insp.","EGCS system-Main engine Quencher bellow was found leaking at several places","E/R - Main Engine,Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Leakages Rectified by tightening compensator Bolts which were found loose ","2022-11-30T23:59:35","","Completed","2022-11-27T23:59:35","No","No","No","Internal",""]
[null,null,null,27315,33127,"0_Sun Oct 30 2022 04:40:57 GMT+0800","2022-10-13T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","One of the crew laundry dryer is defective ","Elect. Mach. & Equip.,Miscellaneous","MLC Related","Equipment Related","11.10","Medium","","","RCVD NEW complete dryer at Cartagena, installed same and found operated satisfactory.","2023-02-13T23:59:35","BCIA230018","Completed","2023-02-06T23:59:35","No","No","No","Internal"]
[null,null,null,27313,17990,"0_Sun Oct 30 2022 04:18:01 GMT+0800","2022-10-18T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","Service air compressor was found not building network pressure ","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","after investigation found pilot air flexible hose ruptured same replaced with temporary copper pipe. Also found air intake assembly defective seal rings and discharge valve assembly.  Found working satisfactory","2023-01-13T23:59:35","BCIA220221","Completed","2022-10-20T23:59:35","No","No","No","Internal"]
[null,null,null,27316,34626,"106_Sun Oct 30 2022 04:33:00 GMT+0800","2022-10-26T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Ships BA compressor transmission belt found damaged . ","LSA / FFA,Miscellaneous","Safety / LSA / FFA","Equipment Related","5.43","High","","","Spare V-belt received and replaced . Tried out working satisfactory","2022-12-26T23:59:35","BCIA220223\nBCIA220224","Completed","2022-10-31T23:59:35","No","No","No","Internal"]
[null,null,null,24668,null,"106_17/3/2022 12:14:27 PM","2022-11-13T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Bunker tank overfill sound horn on midship port and stbd defective","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.8","Medium","","","Bunker tank High level sound horn on midship port and stbd set  to trigger on both high level and overfill alarm. Received strobe light 2 pcs under RO BCIA220052, awaiting maker response regarding supply of horn.","2023-02-12T23:59:35","BCIA225030","Completed",null,"No","No","No","Internal","Spares connected to vessel at Bilboa/Panama on 22nd Dec.as discussed with vessel it will be carried when weather is good"]
[null,null,null,28494,42095,"106_Tue Jan 17 2023 01:36:15 GMT+0800","2022-11-22T23:59:35","Defect","Ship Staff","Ship Staff Insp.","During AE No.3 running found LO high temperature alarm was getting activated ","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Investigated found LO temperature control thermostatic element was defective. Replaced with the spare Thermostatic element. Found working satisfactory ","2023-01-25T23:59:35","","Completed","2022-11-22T23:59:35","No","No","No","Internal"]
[null,null,null,28496,69647,"106_Tue Jan 17 2023 02:03:00 GMT+0800","2022-11-28T23:59:35","Defect","Ship Staff","Ship Staff Insp.","During rounds found No.3 AE Fuel oil leakage alarm was getting activated","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Found Unit No.3 High pressure pipe minor leak was found . Replaced High pressure pipe with new spare pipe. No more leak found working satisfactory ","2023-01-29T23:59:35","","Completed","2022-11-28T23:59:35","No","No","No","Internal"]
[null,null,null,29007,91802,"106_Sat Feb 18 2023 21:30:47 GMT+0800","2022-11-29T23:59:35","Defect","Ship Staff","Ship Staff Insp.","During rounds observed the SW Pressure Inlet to Sox Scrubber ME was Showing incorrect value from the actual inlet pressure. ","E/R - Main Engine,Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Found pressure transmitter 0~6 bars 4-20 mA G1/2\" was showing incorrect value. Received 2 Pc's spare transmitter at Cartagena call. Replaced the same , Found Values Satisfactory.","2023-02-27T23:59:35","BCIA220247","Completed","2023-02-07T23:59:35","No","No","No","Internal"]
[null,null,null,29006,82107,"106_Sat Feb 18 2023 21:20:00 GMT+0800","2022-12-03T23:59:35","Defect","Ship Staff","Ship Staff Insp.","During Exit from Hawaii Found ME EGB Bypass Valve behaving erratic ","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Investigated , found I/P Positioner defective. Received complete Positioner at Cartagena. Replaced the same , Calibrated , Found working satisfactory ","2023-03-03T23:59:35","BCIA 225043","Completed","2023-02-06T23:59:35","No","No","No","Internal"]
[null,null,null,29010,58820,"106_Sat Feb 18 2023 22:05:04 GMT+0800","2022-12-08T23:59:35","Defect","Ship Staff","Ship Staff Insp.","During rounds was observed No.1 AE T/C inlet exh gas temperature digital indicator was showing no value while AE was running ","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Found Digital temperature indicator faulty. Replaced with new spare digital thermometer received at Cartagena. Found Working satisfactory ","2023-03-08T23:59:35","BCIA220237","Completed","2023-02-09T23:59:35","No","No","No","Internal"]
[null,null,null,29008,70870,"106_Sat Feb 18 2023 21:41:54 GMT+0800","2022-12-13T23:59:35","Defect","Ship Staff","Ship Staff Insp.","During Garbage Segregation , found Garbage Compactor was giving operational problem","Miscellaneous,Elect. Mach. & Equip.","General Appearance","Equipment Related","6.20","Medium","","","Found No Signal from main PLC unit to initiate garbage compacting operation , confirmed defective PLC module, received spare PLC Module programmed at Cartagena , Replaced the same, working satisfactory ","2023-03-13T23:59:35","BCIA220229","Completed","2023-02-13T23:59:35","No","No","No","Internal"]
[null,null,null,28503,92049,"106_Tue Jan 17 2023 02:06:15 GMT+0800","2022-12-16T23:59:35","Defect","Ship Staff","Ship Staff Insp.","During Starting of AE No.2. Found Start Fail on AE No.2","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Found Starting air line reducer diaphragm reducer assembly , piston O-ring was defective. Replaced with whole spare assembly . Found working satisfactory ","2023-01-29T23:59:35","","Completed","2022-12-16T23:59:35","No","No","No","Internal"]
[null,null,null,29005,99232,"106_Sat Feb 18 2023 21:24:12 GMT+0800","2022-12-18T23:59:35","Defect","Ship Staff","Ship Staff Insp.","During Passage Found Main Engine LDCL Pump stopped and LDCL system Failure Alarm activated on MOP, Also Found Alarms for 3-way valve supervision failure .","E/R - Main Engine,E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Investigated , found I/P positioner Pneumatic modulating block was defective. Received new modulating block at Cartagena , Replaced the same. Re Calibrated and Initialized the Controller. Found working satisfactory","2023-03-18T23:59:35","BCIA225043","Completed","2023-02-07T23:59:35","No","No","No","Internal"]
[null,null,null,28497,37860,"106_Tue Jan 17 2023 01:32:28 GMT+0800","2022-12-30T23:59:35","Defect","Ship Staff","Ship Staff Insp.","During routine testing of Bunker Tank alarms, found Bunker tank overfill strobe electric hooter alarm on port side mid ship was not sounding","Miscellaneous,Elect. Mach. & Equip.","Emgcy. Systems","Equipment Related","8.14","Very High","","","Found Strobe unit defective. Received complete new strobe unit. Replaced the same , found working satisfactory ","2023-01-24T23:59:35","","Completed","2023-01-15T23:59:35","No","No","No","Internal"]
[null,null,null,29011,54913,"106_Sat Feb 18 2023 22:41:03 GMT+0800","2023-01-04T23:59:35","Defect","Ship Staff","Ship Staff Insp.","During rounds observed No.2 AE No.4 Unit Exhaust gas temperature digital indicator was showing no value ","E/R - Aux. Mach.,E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Found Digital indicator defective, replaced with spare. Digital thermometer received at Cartagena. working satisfactory ","2023-03-29T23:59:35","BCIA220237","Completed","2023-02-09T23:59:35","No","No","No","Internal"]
[null,null,null,28490,12544,"106_Tue Jan 17 2023 01:59:47 GMT+0800","2023-01-15T23:59:35","Defect","Ship Staff","Ship Staff Insp.","During rounds found No.2 Deck Seal Pump was not Building up pressure","E/R - Pipes/ valves & fittings,Inert Gas","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","On investigation found that No.1 Deck Seal Discharge SDNR valve seat was getting stuck causing No.1 pump to rotate in reverse direction causing drop in pressure of No.2 pump. Closed the discharge valve. Found discharge pressure satisfactory. Will overhaul the discharge valve. \non 21 Jan valve removed and overhauled, working satisfactory ","2023-02-26T23:59:35","","Completed","2023-01-19T23:59:35","No","No","No","Internal"]
[null,null,null,29696,85539,"106_Mon Apr 03 2023 15:06:30 GMT+0800","2023-02-06T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","During Supriendentent inspection rounds it was observed that Stencil for Mooring Area was missing on Poop Deck port side.","Miscellaneous","Mooring","Human Error","9.8","Medium","","","Stenciling  was done for \"MOORING AREA\" on poop deck port side.","2023-04-07T23:59:35","NA","Completed","2023-02-09T23:59:35","No","No","No","Internal"]
[null,null,null,29697,26757,"106_Mon Apr 03 2023 15:15:21 GMT+0800","2023-02-06T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Mooring tails 8 nos. found elongated more than the permitted limits as detailed in MSMP & LMP.","Deck - Mooring Machinery","Mooring","Equipment Related","9.5","High","","","Mooring tails 8 nos. renewed with new tails.","2023-05-07T23:59:35","BCIA230007","Completed","2023-03-22T23:59:35","No","No","No","Internal"]
[null,null,null,29004,14593,"106_Sat Feb 18 2023 22:46:20 GMT+0800","2023-02-07T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","During Cargo discharging at Cartagena , found Vacuum pressure transmitter for COPT vacuum condenser sending signal to AMS was showing frozen value comparing with the  actual local vacuum gauge value .  ","E/R - Aux. Mach.,Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Investigated , removed pressure transmitter , found choked with deposits, same cleaned and calibrated and found values satisfactory and no error ","2023-05-15T23:59:35","","Completed","2023-03-01T23:59:35","No","No","No","Internal"]
[null,null,null,29009,28666,"106_Sat Feb 18 2023 21:55:55 GMT+0800","2023-02-07T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Noted during UMS period Bilge well high level alarm port side was activated, Found No.2 EGCS SW Pump NRV Flap got ruptured causing water splash. ","E/R - Pipes/ valves & fittings,E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Replaced NRV Flap valve with spare new flap valve received at Cartagena, Tried out working Satisfactory  ","2023-05-12T23:59:35","BCIA230037","Completed","2023-02-12T23:59:35","No","No","No","Internal"]
[null,null,null,29695,51891,"106_Sat Apr 01 2023 22:33:05 GMT+0800","2023-03-03T23:59:35","Defect","Ship Staff","Ship Staff Insp.","AE No.2 Unit No.6 Exhaust gas digital thermometer found defective ","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Replaced thermometer with new spare thermometer ","2023-06-03T23:59:35","","Completed","2023-03-03T23:59:35","No","No","No","Internal"]
[null,null,null,29692,61127,"106_Sat Apr 01 2023 22:20:27 GMT+0800","2023-03-07T23:59:35","Defect","Ship Staff","Ship Staff Insp.","During rounds found No.2 Provision Compressor oil leakage from Shaft Seal ","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Replaced Shaft Seal with new spare. Leakage rectified and raised RO for spare Set of seal ","2023-06-07T23:59:35","BCIA230090","Completed","2023-03-10T23:59:35","No","No","No","Internal"]
[null,null,null,29694,55949,"106_Sat Apr 01 2023 22:27:28 GMT+0800","2023-03-09T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Main air compressor No.2 1st stage safety valve started lifting ","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Investigated found 2nd Stage Valve defective . replaced with new spare. Found working satisfactory ","2023-05-30T23:59:35","","Completed","2023-03-09T23:59:35","No","No","No","Internal"]
[null,null,null,30159,10316,"106_Sat May 06 2023 04:38:13 GMT+0800","2023-03-11T23:59:35","Defect","Ship Staff","Ship Staff Insp.","FUNNEL FLAPS LOCAL PNEUMATIC VALVE FOUND IN OPERATIVE","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","VESSEL RECEIVED THE SPARE AND RENWED THE PNEUMATIC VALVE, CHECKED FLAP OPERATION FOUND SATISFACTORY","2023-06-11T23:59:35","BCIA235002","Completed","2023-04-13T23:59:35","No","No","No","Internal"]
[null,null,null,29691,90271,"106_Sat Apr 01 2023 22:16:28 GMT+0800","2023-03-21T23:59:35","Defect","Ship Staff","Ship Staff Insp.","During Inspection of Incinerator furnace found sluice door one of the ceramic board plate was found broken","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Replaced with spare ceramic plate with securing bolts and oval washer. raised RO for spare ceramic board plate ","2023-06-21T23:59:35","BCIA230107","Completed","2023-03-22T23:59:35","No","No","No","Internal"]
[null,null,null,29693,53506,"106_Sat Apr 01 2023 22:23:35 GMT+0800","2023-03-25T23:59:35","Defect","Ship Staff","Ship Staff Insp.","ME FO Circulating pump No.2 found leakage from Shaft seal ","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Replaced shaft seal and bearing with new spare. Leakage rectified. Raise RO for spare overhaul Kit also","2023-04-25T23:59:35","BCIA230108","Completed","2023-03-25T23:59:35","No","No","No","Internal"]
[null,null,null,30186,40721,"106_Tue May 30 2023 03:18:39 GMT+0800","2023-04-02T23:59:35","Defect","Ship Staff","Ship Staff Insp.","MAIN ENGINE EGCS INLET BELLOW FOUND DAMAGED. GAS AND WATER WAS LEAKING.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.3","Medium","","","VESSEL RECEIVED THE BELLOW IN TRIESTE UNDER PO NO BCIA220169. SAME RENEWED. LAGGING RENEWED.","2023-07-02T23:59:35","BCIA220169","Completed","2023-05-22T23:59:35","No","No","No","Internal"]
[null,null,null,30157,12009,"106_Sat May 06 2023 04:55:33 GMT+0800","2023-04-14T23:59:35","Defect","Ship Staff","Ship Staff Insp.","BRIDGE AIR CONDITIONING UNIT BLOWER BEARING FOUND  NOISY .","Miscellaneous","General Appearance","Equipment Related","10.3","Medium","","","VESSEL RECEIVED THE BEARING UNDER PO BCIA230138 AND  REPLACED THE BEARINGS AND TRIED OUT THE SAME, WORKING SATISFACTORY.","2023-09-02T23:59:35","","Completed","2023-08-23T23:59:35","No","No","No","Internal"]
[null,null,null,30160,14104,"106_Sat May 06 2023 04:47:41 GMT+0800","2023-04-15T23:59:35","Defect","Ship Staff","Ship Staff Insp.","COMPOSITE BOILER COMBUSTION FAN SERVO MOTOR FOUND IN-OPERATIVE DURING OPERATION","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.3","Medium","","","VESSEL RENEWED COMPOSITE BOILER COMBUSTION FAN SERVO MOTOR WITH NEW SPARE ON BOARD. COMPOSITE BOILER TRIED OUT FOUND WORKING SATISFACTORY.","2023-07-15T23:59:35","BCIA230115","Completed","2023-04-15T23:59:35","No","No","No","Internal"]
[null,null,null,30158,40531,"106_Sat May 06 2023 04:42:00 GMT+0800","2023-04-18T23:59:35","Defect","Ship Staff","Ship Staff Insp.","NO 2 AUX BOILER SMOKE DENSITY METER SHOWING ERROR CODE \"LOC\"- TRNSMITTER LAMP INTENSITY REDUCED. ","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","SPARE SMOKE DENSITY METER TRANSMITTER PCB CARD WAS RCVD ON BOARD,SAME INSTALLAED IN PLACE-PRESENTLY OPERATED SATISFACTORY.","2023-07-18T23:59:35","BCIA230116","Completed","2023-07-23T23:59:35","No","No","No","Internal"]
[null,null,null,30187,37080,"106_Tue May 30 2023 03:20:44 GMT+0800","2023-05-21T23:59:35","Defect","Ship Staff","Ship Staff Insp.","MAIN ENGINE EGCS INLET SIDE QUENCHER PIPE FOUND BROKEN AND DAMAGED","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related","10.3","Medium","","","VESSEL FABRICATED THE QUENCHER PIPE SECTION WITH SPARE NEW PIPE. SAME FITTED BACK AND TRIED OUT THE SYSTEM.","2023-08-21T23:59:35","","Completed","2023-05-23T23:59:35","No","No","No","Internal"]
[null,null,null,30184,92322,"106_Tue May 30 2023 04:12:03 GMT+0800","2023-05-30T23:59:35","Defect","Ship Staff","Ship Staff Insp.","HFO SERVICE TANK TEMPERATURE CONTROLLER CAPILLARY TUBE DAMAGED.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.3","Medium","","","Newly received controller fitted in place ,working satisfactory.","2023-08-30T23:59:35","BCIA230140","Completed","2023-09-15T23:59:35","No","No","No","Internal"]
[null,null,null,30185,27154,"106_Tue May 30 2023 02:40:01 GMT+0800","2023-05-30T23:59:35","Defect","Ship Staff","Ship Staff Insp.","AUX BOILER NO 2 STEAM STOP VALVE BONNET AND SPINDLE DAMAGED.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.3","Medium","","","VESSEL RECEIVED THE SPARE BONNET AND SPINDLE IN HOUSTON. SAME REPLACED","2023-08-30T23:59:35","BCIA230046","Completed","2023-05-30T23:59:35","No","No","No","Internal"]
[null,null,null,31275,32427,"106_Tue Jun 27 2023 16:28:18 GMT+0800","2023-06-23T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","No records available for calibration of the BHC test kit pressure gauge","Documentation","Mooring","Inappropriate Procedure","9.7","Medium","","","PRESSURE CALIBRATION OF BHC KIT PRESSURE GUAGE CARRIED OUT WITH ONBOARD CALIBRATOR ( RANGE UPTO 700 BARS ). FOUND SATISFACTORY.","2023-09-22T23:59:35","","Completed","2023-08-21T23:59:35","No","No","No","Internal"]
[null,null,null,31276,67482,"106_Tue Jun 27 2023 15:42:41 GMT+0800","2023-06-23T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","PV Valve last test is May 2020, Vessel does not have a test bench on board.","Deck - Pipe / Fittings","Cargo / Ballast Systems","Equipment Related","8.21","High","","","VESSEL FOUND PV VALVE TEST KIT & SPARE PV VALVE FOR TESTING. KEPT IN STBD SIDE MIDSHIP SOTRE.","2023-12-17T23:59:35","BCIA230171","Completed","2023-08-11T23:59:35","No","No","No","Internal"]
[null,null,null,31277,71374,"106_Tue Jun 27 2023 16:17:24 GMT+0800","2023-06-23T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Batteries of 12 locations on board are overdue for replacement in March 2023","Miscellaneous","Emgcy. Systems","Equipment Related","10.37","Medium","","","VESSEL RECEIVED BATTERIES UNDER PO BCIA230139 AND REPLACEED ALL BATEERIES .","2023-08-22T23:59:35","BCIA230139","Completed","2023-08-26T23:59:35","No","No","No","Internal"]
[null,null,null,31278,61581,"106_Tue Jun 27 2023 21:37:28 GMT+0800","2023-06-23T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Strip and wax mess room floors","Accommodation","MLC Related","Human Error","11.13","Low","","","CREW & OFFICERS MESSROOMS STRIPPED & POLISHED.","2023-08-22T23:59:35","BCIA230174","Completed","2023-08-22T23:59:35","No","No","No","Internal"]
[null,null,null,31279,98084,"106_Tue Jun 27 2023 21:39:43 GMT+0800","2023-06-23T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Fabricate shelves in the laundries (in line with Good practices circulars) to deter crew from placing clothes on the washing machines and dryers.","Accommodation","MLC Related","Human Error","11.14","Medium","","","SHELVES INSTALLED IN CREW & OFFICERS LAUNDRY.","2023-09-22T23:59:35","","Completed","2023-08-28T23:59:35","No","No","No","Internal"]
[null,null,null,31280,67960,"106_Mon Jul 24 2023 11:42:47 GMT+0800","2023-06-23T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Vessel Does not have spare light shades for the pumproom (6Nos)","Elect. Mach. & Equip.","ISM Related","Equipment Related","","","","","Vessel received spare.","2023-08-23T23:59:35","BCIA230193","Completed","2023-09-14T23:59:35","No","No","No","Internal"]
[null,null,null,31282,21574,"106_Tue Jun 27 2023 16:37:37 GMT+0800","2023-06-23T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Mooring lines from W1 inner and W2 inner drums chaffing at the 64 T fairlead rope guide bar prior passing through the leads","Deck - Mooring Machinery","Mooring","Equipment Related","9.18","Low","","","Vessel checked and confirmed that the wire is passing  between the guide bar & the roller with a direct lead.","2025-07-22T23:59:35","","Completed","2023-08-12T23:59:35","No","No","No","Internal"]
[null,null,null,31283,63979,"106_Tue Jun 27 2023 18:02:07 GMT+0800","2023-06-23T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Manifold drip tray grating frames to be buffed and re painted at locations where corrosion starting (Below frames/ supports)","Deck - Pipe / Fittings","General Appearance","","","","","","Port & stbd side manifold  drip trays & their gratings chipped, buffed and  painted.","2023-08-22T23:59:35","","Completed","2023-08-29T23:59:35","No","No","No","Internal"]
[null,null,null,31284,45223,"106_Tue Jun 27 2023 18:04:15 GMT+0800","2023-06-23T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","COW machine branch valves have some stud eroded, To carry out surface preparation and paint","Deck - Pipe / Fittings","Cargo / Ballast Systems","Human Error","8.34","High","","","ALL COW MACHINE BRANCH VALVES CHIPPED , BUFFED & PAINTED.","2023-08-22T23:59:35","","Completed","2023-08-22T23:59:35","No","No","No","Internal"]
[null,null,null,31285,47305,"106_Tue Jun 27 2023 21:23:12 GMT+0800","2023-06-23T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Steam line to de-rust and paint with Red HR paint (Kindly discuss scheme with Nikitas/ Gloria Maris)","Deck - Pipe / Fittings","General Appearance","Equipment Related","","","","","Paints received in Singapore. Derusting & painting completed","2024-03-17T23:59:35","BCIA230181","Completed","2024-03-01T23:59:35","No","No","No","Internal","13/2 - please update the job as the target date was in Nov 2023. if any extnsion is required, same to be informed / requested\n\n20/02 - please udpate reasons. target date is way overdue.  Moving the target date to 15 March."]
[null,null,null,31286,92687,"106_Tue Jun 27 2023 21:33:53 GMT+0800","2023-06-23T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Pumproom Void space to be drained and cleaning to be carried out, as few rust spots to be attended to","Miscellaneous","Cargo / Ballast Systems","Human Error","","","","","P/ROOM BOTTOM PLATFORM CLEANED & PAINTED. VOID SPACE BROOMED & MOPPED.","2023-09-22T23:59:35","","Completed","2023-08-28T23:59:35","No","No","No","Internal"]
[null,null,null,31287,95531,"106_Tue Jun 27 2023 16:24:28 GMT+0800","2023-06-23T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Liberian certificates of Officers and engineers to be displayed in a common location","Documentation","Cert. & Docu.","Human Error","3.5","Medium","","","Liberian certificates of Officers and engineers displayed on notice board just outside Master cabin. ","2023-07-22T23:59:35","","Completed","2023-06-25T23:59:35","No","No","No","Internal"]
[null,null,null,31288,54616,"106_Tue Jun 27 2023 16:31:02 GMT+0800","2023-06-23T23:59:35","Critical Equipment","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Life boat limit switches to be lubricated as currently sluggish","Critical Equip.","Emgcy. Systems","Equipment Related","4.27","High","","","The Limit switch was free and well lubricated to prevent any sluggish movement. ","2023-07-02T23:59:35","","Completed","2023-06-26T23:59:35","No","No","No","Internal"]
[null,null,null,31289,57948,"106_Tue Jun 27 2023 18:00:31 GMT+0800","2023-06-23T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Pumproom cleaning required","Miscellaneous","Cargo / Ballast Systems","Human Error","","","","","Pumproom cleaned thoroughly. Step marked removed. ","2023-07-22T23:59:35","","Completed","2023-06-23T23:59:35","No","No","No","Internal"]
[null,null,null,31290,66621,"106_Tue Jun 27 2023 21:26:00 GMT+0800","2023-06-23T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Door closer at CCR door to be renewed","Miscellaneous","ISM Related","External Factors","","","","","The door closer is need to be adjusted. The closer has been adjusted. ","2023-07-22T23:59:35","","Completed","2023-06-28T23:59:35","No","No","No","Internal"]
[null,null,null,31291,24184,"106_Tue Jun 27 2023 22:32:38 GMT+0800","2023-06-23T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Vessel has found 4 no.s new coir fenders located at steering gear flat & 2 in use fenders kept in pumpman store.","Miscellaneous","Mooring","Equipment Related","","","","","Found onboard 6 no.s","2023-08-22T23:59:35","","Completed","2023-06-30T23:59:35","No","No","No","Internal"]
[null,null,null,31292,23189,"106_Tue Jun 27 2023 17:01:48 GMT+0800","2023-06-23T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","VRCS local connections and Gas detection system 3 way valves are open to weather and have commenced calcification, recommend cleaning and covering with petroleum tape (denso).","Cargo Mach.","Cargo / Ballast Systems","Inappropriate Procedure","","","","","All VRCS local connections and Gas detection system 3 way valves on deck have been cleaned & covered with petroleum / denso tape.","2023-09-22T23:59:35","","Completed","2023-07-02T23:59:35","No","No","No","Internal"]
[null,null,null,31293,72373,"106_Tue Jun 27 2023 21:20:59 GMT+0800","2023-06-23T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Self lowering wires of the lifeboats to be de- greased and sheeves cleaned as grease is obstructing its passage through the sheaves","LSA / FFA","Safety / LSA / FFA","Human Error","5.27","Medium","","","-Will carryout greasing of Self lowering wires of the lifeboats and sheeves. \n- Greasing and oiling of Self lowering wire and sheeves carried out.  ","2023-07-22T23:59:35","","Completed","2023-07-02T23:59:35","No","No","No","Internal"]
[null,null,null,31294,51382,"106_Tue Jun 27 2023 18:07:47 GMT+0800","2023-06-23T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Stands for Pilot ladder embarkation lights and Life raft embarkation lights (Fwd and aft) frozen, to freeup and lubricate","LSA / FFA","Safety / LSA / FFA","Inappropriate Procedure","5.28","Very High","","","To Free Pilot ladder embarkation light and Life raft lights to be free and lubricate. \n- Completed freeing Pilot ladder light and life raft. ","2023-07-22T23:59:35","","Completed","2023-07-03T23:59:35","No","No","No","Internal"]
[null,null,null,31295,29792,"106_Tue Jun 27 2023 15:59:30 GMT+0800","2023-06-23T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","SEP Annex 1 procedures to be promulgated and stored together either in file or a separate file in line with SEP annex procedures.","Documentation","","Human Error","2.3","High","","","The SEP Annex 1 procedures to include all items as per List provided. \n- Completed SEP file as per list provided on 25th. June","2023-07-22T23:59:35","","Completed","2023-06-27T23:59:35","No","No","No","Internal"]
[null,null,null,31296,68474,"106_Tue Jun 27 2023 17:58:31 GMT+0800","2023-06-23T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Hydraulic leak from the Overboard valve actuator in pumproom, Rectify leak and clean up the areas","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.11","Medium","","","Need to repair leakage of O/B valve actuator. \n- the leakage was due to operating the valve beyond its pressure range. Completed on 30 June 2023","2023-07-22T23:59:35","","Completed","2023-07-02T23:59:35","No","No","No","Internal"]
[null,null,null,31297,91973,"106_Tue Jun 27 2023 22:49:03 GMT+0800","2023-06-23T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Port side Bow stopper Locking pin (Open Position) bent ","Deck - Mooring Machinery","Mooring","Human Error","9.20","Medium","","","Need to remove taken to E/R heated and straighten up. \n- The Pin was straighten up and placed back. ","2023-07-22T23:59:35","","Completed","2023-07-05T23:59:35","No","No","No","Internal"]
[null,null,null,31298,87340,"106_Tue Jun 27 2023 21:28:20 GMT+0800","2023-06-23T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Crew and officers to familiarize and commence operating the remote winch controls which provide additional safety.","Deck - Mooring Machinery","Mooring","Human Error","","","","","To give training to all officers and crew to operate remote winch controls. \n- Training given to crew and officer for remote operation of Winch control. ","2023-08-22T23:59:35","","Completed","2023-07-13T23:59:35","No","No","No","Internal"]
[null,null,null,31299,25833,"106_Tue Jun 27 2023 16:20:43 GMT+0800","2023-06-23T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","2 nos starter panels in the ER are located next to the fire hydrants without adequate protection \n-\tNo 3 group starter panel (outside ECR)\n-\tCOPT vac Condenser p/p","Miscellaneous","MLC Related","Industry Issue","","","","","Vessel fitted acrylic sheet on the No 3 group starter panel (outside ECR) and COPT vac Condenser p/p to give protection against water ingress due to leakage through the adjacent water pipe line.","2023-08-22T23:59:35","","Completed","2023-07-14T23:59:35","No","No","No","Internal"]
[null,null,null,31300,22868,"106_Tue Jun 27 2023 21:17:49 GMT+0800","2023-06-23T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Fairleads (especially on forecastle) to be buffed and painted","Deck - Pipe / Fittings","Mooring","External Factors","9.18","Low","","","V/L will buff and paint Fairlead especially Forecastle. \n- Buffed and painted fairleads on Forecastle. Completed on 15 Jul 23","2023-07-22T23:59:35","","Completed","2023-07-17T23:59:35","No","No","No","Internal"]
[null,null,null,31301,93469,"106_Tue Jun 27 2023 16:34:32 GMT+0800","2023-06-23T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Fwd Hydraulic starter panel cover locking mechanism is loose, to be adjusted to prevent accidental rain/ water entering","Deck - Machinery","Mooring","Human Error","9.16","High","","","Extra Rubber packing placed and now its water tight. ","2023-09-22T23:59:35","","Completed","2023-07-03T23:59:35","No","No","No","Internal"]
[null,null,null,33577,68112,"106_Tue Jan 16 2024 15:44:42 GMT+0800","2023-08-13T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Steering gear entrance from ER, sealing lagging to slight damaged at some place.","E/R - Pipes/ valves & fittings","Safety / LSA / FFA","External Factors","","","","","Steering gear entrance from ER, sealing lagging to slight damaged at some place, same has been replaced.","2023-08-15T23:59:35","","Completed","2023-08-14T23:59:35","No","No","No","Internal"]
[null,null,null,33578,64052,"106_Tue Jan 16 2024 15:48:18 GMT+0800","2023-08-13T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Oil traces below DG#2 & 3 flywheel need to be cleaned","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","","","","","Oil traces below DG#2 & 3 flywheel  cleaned","2023-08-15T23:59:35","","Completed","2023-08-14T23:59:35","No","No","No","Internal"]
[null,null,null,33579,82230,"106_Tue Jan 16 2024 15:54:53 GMT+0800","2023-08-13T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Some emergency lights in accommodation & Pump room found fused.","Elect. Mach. & Equip.","Emgcy. Systems","Equipment Related","","","","","Fused emergency lights in accommodation &  pump room  replaced with new lights","2023-08-15T23:59:35","","Completed","2023-08-15T23:59:35","No","No","No","Internal"]
[null,null,null,33580,11329,"106_Tue Jan 16 2024 15:35:30 GMT+0800","2023-08-13T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Change request  form for deck air compressor need to be sent with change in PMS schedule","Documentation","Cert. & Docu.","Human Error","","","","","Change request  form for deck air compressor  sent with change in PMS schedule","2023-08-28T23:59:35","","Completed","2023-08-18T23:59:35","No","No","No","Internal"]
[null,null,null,33581,60861,"106_Tue Jan 16 2024 15:57:30 GMT+0800","2023-08-13T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Some deck lights electric connection union has gaps & need to be filled with electrical putty.","Elect. Mach. & Equip.","General Appearance","Equipment Related","","","","","Deck lights electric connection union  gaps  filled with electrical putty.","2023-08-15T23:59:35","","Completed","2023-08-14T23:59:35","No","No","No","Internal"]
[null,null,null,33582,34066,"106_Tue Jan 16 2024 16:07:23 GMT+0800","2023-08-13T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","FWD & AFT hydraulic oil tank to be cleaned on 6 months basis, Send CRF to add this job in PAL","Deck - Machinery,Documentation","Cert. & Docu.","Equipment Related","","","","","FWD & AFT hydraulic oil tank to be cleaned on 6 months basis, Sent CRF to add this job in PAL.","2023-09-13T23:59:35","","Completed","2023-09-07T23:59:35","No","No","No","Internal"]
[null,null,null,33583,55453,"106_Tue Jan 16 2024 16:10:49 GMT+0800","2023-08-13T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Exhaust pipe for laundry dryer to be cover with specific high temperature resistance tape.","Accommodation","General Appearance","Equipment Related","","","","","Exhaust pipe for laundry dryer  covered with specific high temperature resistance tape.","2023-09-28T23:59:35","","Completed","2023-09-04T23:59:35","No","No","No","Internal"]
[null,null,null,33584,36596,"106_Tue Jan 16 2024 18:29:11 GMT+0800","2023-08-13T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","All spares received on deck to be secure with wire ropes.","Miscellaneous","General Appearance","Human Error","","","","","All spares received on deck  secured with wire ropes.","2023-08-14T23:59:35","","Completed","2023-08-14T23:59:35","No","No","No","Internal"]
[null,null,null,31281,86817,"106_Tue Aug 15 2023 17:12:36 GMT+0800","2023-08-13T23:59:35","Observation","Ship Staff","Ship Staff Insp.","AUX ENGINE EGCS SCRUBBER QUENCHER ONE SECTION PIPE GOT HOLED.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.3","Medium","","","VESSEL RECEIVED SPARE PIPE AND FLANGES, NEW PIPE FABRICATED AND FITTED BACK AND TRIED OUT.","2023-10-13T23:59:35","BCIA230197","Completed","2023-08-26T23:59:35","No","No","No","Internal"]
[null,null,null,33585,94756,"106_Tue Jan 16 2024 15:38:39 GMT+0800","2023-08-13T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","MSDS to be posted near Calibration/Freon bottles  on first platform","Documentation","Cert. & Docu.","Human Error","","","","","MSDS  posted near Calibration/Freon bottles  on first platform","2023-08-15T23:59:35","","Completed","2023-08-14T23:59:35","No","No","No","Internal"]
[null,null,null,33586,25337,"106_Tue Jan 16 2024 16:03:40 GMT+0800","2023-08-13T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ME SCR new foundation fitting job to be reported in Refman for  carrying out job in next drydock","Documentation","Cert. & Docu.","Knowledge Based","","","","","ME SCR new foundation fitting job  reported in Refman for  carrying out job in next drydock","2023-09-13T23:59:35","","Completed","2023-09-07T23:59:35","No","No","No","Internal"]
[null,null,null,33587,91345,"106_Tue Jan 16 2024 18:35:52 GMT+0800","2023-08-13T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","All steam line valves on deck found to be rusted again, same to be de-rusted and painted.","Deck - Machinery","General Appearance","Equipment Related","","","","","All steam line valves on deck der-rusted and painted with high temperature aluminum paint.","2023-11-02T23:59:35","","Completed","2023-09-13T23:59:35","No","No","No","Internal"]
[null,null,null,33588,85953,"106_Tue Jan 16 2024 18:40:43 GMT+0800","2023-08-13T23:59:35","Observation","Ship Staff","Suptd. Insp.","IMO symbol on port side midship locker weathertight  door found faded, same to be replaced with new one.","Miscellaneous","Cert. & Docu.","External Factors","","","","","IMO symbol on port side midship locker weathertight door replaced with new one.","2023-09-13T23:59:35","","Completed","2023-09-09T23:59:35","No","No","No","Internal"]
[null,null,null,33589,81146,"106_Tue Jan 16 2024 19:51:24 GMT+0800","2023-08-13T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Helicopter equipment's to be shifted to separate location ,should be easily accessible.","Deck - Machinery","General Appearance","Knowledge Based,External Factors","","","","","Helicopter equipment's  shifted to port side midship locker.","2023-10-13T23:59:35","","Completed","2023-09-13T23:59:35","No","No","No","Internal"]
[null,null,null,33590,30352,"106_Tue Jan 16 2024 19:53:53 GMT+0800","2023-08-13T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Anti-piracy hoses to be marked and kept at specific location.","Deck - Pipe / Fittings","General Appearance","Equipment Related","","","","","Anti-piracy hoses  marked and kept in midship locker.","2023-09-13T23:59:35","","Completed","2023-09-08T23:59:35","No","No","No","Internal"]
[null,null,null,33591,33112,"106_Tue Jan 16 2024 19:57:03 GMT+0800","2023-08-13T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","All embarkation ladder connecting shackle & exposed ropes to be greases. ","Deck - Pipe / Fittings","General Appearance","Equipment Related","","","","","All embarkation ladder connecting shackle & exposed ropes greases. ","2023-09-28T23:59:35","","Completed","2023-09-13T23:59:35","No","No","No","Internal"]
[null,null,null,33592,29273,"106_Tue Jan 16 2024 19:59:17 GMT+0800","2023-08-13T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","All lifebuoys to be painted with fire retardant paint ","LSA / FFA","Safety / LSA / FFA","External Factors","","","","","All lifebuoys painted with fire retardant paint .","2023-11-01T23:59:35","","Completed","2023-10-02T23:59:35","No","No","No","Internal"]
[null,null,null,33593,65981,"106_Tue Jan 16 2024 20:06:09 GMT+0800","2023-08-13T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Windlass brake band tightening  screw to be cleared ( At least 2 mm clearance to be maintain)","Deck - Machinery","Mooring","Equipment Related","","","","","Windlass brake band tightening  screw adjusted to maintain 2 mm clearance.","2023-09-13T23:59:35","","Completed","2023-09-11T23:59:35","No","No","No","Internal"]
[null,null,null,33594,38951,"106_Tue Jan 16 2024 20:13:35 GMT+0800","2023-08-13T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","One of the wooden step on stbd side pilot ladder found slightly damaged & bottom rubber step shape deformed. Ladder to be replaced with new & this type repair kit to be ordered.","Deck - Pipe / Fittings","General Appearance","Equipment Related","","","","","One of the wooden step on stbd side pilot ladder found slightly damaged , ladder has been replaced with new ladder, Repair kit has been ordered.","2023-09-13T23:59:35","","Completed","2023-09-09T23:59:35","No","No","No","Internal"]
[null,null,null,33595,70721,"106_Tue Jan 16 2024 20:17:54 GMT+0800","2023-08-13T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","PV valve test kit to be checked & tested in ballast passage. Both PV valves kept in same location.","Miscellaneous","Cargo / Ballast Systems","Equipment Related","","","","","PV valve test kit  checked & tested  during ballast passage. PV valve shifted to two different locations & secured.","2023-09-13T23:59:35","","Completed","2023-09-12T23:59:35","No","No","No","Internal"]
[null,null,null,33596,78014,"106_Tue Jan 16 2024 20:22:04 GMT+0800","2023-08-13T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Poop deck L/buoy light covered with spot paint. Same to be removed.","","Safety / LSA / FFA","Human Error","","","","","Poop deck L/buoy light covered with spot paint. Same paint cleaned.","2023-08-28T23:59:35","","Completed","2023-08-20T23:59:35","No","No","No","Internal"]
[null,null,null,33597,30795,"106_Tue Jan 16 2024 20:25:53 GMT+0800","2023-08-13T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","L/buoy grab line certificate to be checked for \"Non kinking type\"","Documentation","Cert. & Docu.","Knowledge Based","","","","","L/buoy grab line certificate checked for \"Non kinking type\"","2023-08-18T23:59:35","","Completed","2023-08-16T23:59:35","No","No","No","Internal"]
[null,null,null,33598,36827,"106_Tue Jan 16 2024 20:02:24 GMT+0800","2023-08-13T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Anchor hawse pipe to be covered during anchorage as per ISPS measures.","Miscellaneous","General Appearance","Knowledge Based","","","","","Anchor hawse pipe  covered during anchorage as per ISPS measures.","2023-08-16T23:59:35","","Completed","2023-08-15T23:59:35","No","No","No","Internal"]
[null,null,null,33599,21286,"106_Tue Jan 16 2024 20:08:41 GMT+0800","2023-08-13T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Old & condemned ladder on FPK store to be tagged .","Miscellaneous","Safety / LSA / FFA","Knowledge Based","","","","","Old & condemned ladder on FPK store  tagged  & secured.","2023-09-13T23:59:35","","Completed","2023-09-06T23:59:35","No","No","No","Internal"]
[null,null,null,33600,10597,"106_Tue Jan 16 2024 18:32:01 GMT+0800","2023-08-13T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Port side life boat davit limit switch found to be frozen, same need to be overhauled & made free","Deck - Machinery","Safety / LSA / FFA","Equipment Related","","","","","Port side life boat davit limit switch overhauled and made free.","2023-08-14T23:59:35","","Completed","2023-08-14T23:59:35","No","No","No","Internal"]
[null,null,null,32647,45057,"106_Sat Sep 30 2023 16:17:52 GMT+0800","2023-09-25T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Cargo oil tank 3 Stbd Temp. sensor is defective","Elect. Mach. & Equip.","Cargo / Ballast Systems","Equipment Related","8.13","Medium","","","Sensor interchanged to check  and verify with COT 3 Port as per office instructions. Correspondence with office is in progress. Sensor is operational now","2023-12-25T23:59:35","","Completed","2023-11-29T23:59:35","No","No","No","Internal"]
[null,null,null,32649,95606,"106_Sat Sep 30 2023 16:51:52 GMT+0800","2023-09-27T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","Portable gas meter is not switching on.\nMake: MSA\nModel: Altair 5XIR\nSerial no.: 06010643\n","Miscellaneous","Safety / LSA / FFA","Equipment Related","5.23","Very High","","","Service provider informed ,Equipment will be replaced at convenient port. \n16th Oct-2023- Vessel received new Gas meter at Piraeus","2023-12-27T23:59:35","","Completed","2023-10-18T23:59:35","No","No","No","Internal"]
[null,null,null,32648,44249,"106_Tue Oct 31 2023 19:38:01 GMT+0800","2023-10-23T23:59:35","Defect","Ship Staff","Ship Staff Insp.","IG  PLATFORM AREA  IN E/R -\"O2 SENSOR DEFECTIVE \",NEED REPLACEMENT.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","8.30","High","","","Spare sensor received and replaced, not oxygen sensor is operational","2024-01-22T23:59:35","BCIA230224","Completed","2023-12-04T23:59:35","No","No","No","Internal"]
[null,null,null,33402,94683,"106_Thu Jan 11 2024 17:57:32 GMT+0800","2023-11-29T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Port lifeboat davit limit switch to be cleaned of salt deposits and freed","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","Port lifeboat davit limit switch cleaned of salt deposits and freed","2023-12-06T23:59:35","","Completed","2023-11-30T23:59:35","No","No","No","Internal"]
[null,null,null,33403,95995,"106_Thu Jan 11 2024 18:00:34 GMT+0800","2023-11-29T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Water accumulated in port lifeboat at of the drain plug to be cleaned","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","Cleaned on 28 Nov 2023","2023-12-06T23:59:35","","Completed","2023-11-30T23:59:35","No","No","No","Internal"]
[null,null,null,33404,40382,"106_Thu Jan 11 2024 18:02:53 GMT+0800","2023-11-29T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Oxygen and acetylene room safety posters to be renewed","Miscellaneous","ISM Related","Human Error","","","","","Oxygen and acetylene room safety posters  renewed","2023-12-09T23:59:35","","Completed","2023-12-02T23:59:35","No","No","No","Internal"]
[null,null,null,33405,40306,"106_Thu Jan 11 2024 18:05:37 GMT+0800","2023-11-29T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","2 Spare belts for the lifeboat to be ordered","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","BCIA240006 Raised, old one was cancelled as per the instruction from the procurement ","2024-01-09T23:59:35","","Completed","2024-01-07T23:59:35","No","No","No","Internal"]
[null,null,null,33406,73309,"106_Thu Jan 11 2024 18:05:54 GMT+0800","2023-11-29T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","All EGCS ovbd pipe stub pieces to be painted & below area to be cleaned, stem lagging where damaged need to be repaired. ","E/R - Pipes/ valves & fittings","General Appearance","Equipment Related","","","","","All EGCS ovbd pipe stub pieces  painted & below area  cleaned, stem lagging where damaged renewed with new lagging","2023-12-06T23:59:35","","Completed","2023-12-02T23:59:35","No","No","No","Internal"]
[null,null,null,33407,13697,"106_Thu Jan 11 2024 17:57:36 GMT+0800","2023-11-29T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Malfunctioning Emergency lights in pump room to be replaced with new lights     ","Elect. Mach. & Equip.","General Appearance","Equipment Related","","","","","Defective  Emergency lights in pump room  replaced with new lights     ","2023-12-14T23:59:35","","Completed","2023-12-02T23:59:35","No","No","No","Internal"]
[null,null,null,33408,80886,"106_Thu Jan 11 2024 18:08:12 GMT+0800","2023-11-29T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Pump room damper box to be de-rusted and painted","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","Pump room damper box de-rusted and painted","2023-12-29T23:59:35","","Completed","2023-12-20T23:59:35","No","No","No","Internal"]
[null,null,null,33409,72188,"106_Thu Jan 11 2024 18:08:25 GMT+0800","2023-11-29T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Suspected HFO trans pp vent cock leak, check & rectify tray to be cleaned & painted.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","HFO transfer pump  leaky vent valve renewed with new spare. Save all tray cleaned & painted.","2023-12-06T23:59:35","","Completed","2023-12-01T23:59:35","No","No","No","Internal"]
[null,null,null,33410,78656,"106_Thu Jan 11 2024 18:10:40 GMT+0800","2023-11-29T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Pump room mushroom vent to be de-rusted and painted","Deck - Machinery","Safety / LSA / FFA","Equipment Related","","","","","Pump room mushroom vent de-rusted and painted","2023-12-29T23:59:35","","Completed","2023-12-29T23:59:35","No","No","No","Internal"]
[null,null,null,33411,55403,"106_Thu Jan 11 2024 18:13:07 GMT+0800","2023-11-29T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","AUS drain tank to be drained and cleared of any signs of oil","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","AUS drain tank drained and cleared of any signs of oil","2023-12-29T23:59:35","","Completed","2023-12-05T23:59:35","No","No","No","Internal"]
[null,null,null,33412,36730,"106_Thu Jan 11 2024 18:12:31 GMT+0800","2023-11-29T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Control air compressor makes slight abnormal noise during loading, same to be checked. ","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Control air compressor 8000 hrs. routine carried out. Belt tension checked & auto unloader renewed. Compressor in use , found running normal.","2023-12-14T23:59:35","","Completed","2023-12-03T23:59:35","No","No","No","Internal"]
[null,null,null,33413,71813,"106_Thu Jan 11 2024 18:21:46 GMT+0800","2023-11-29T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Pilot ladder winch lube level to be replenished","Deck - Machinery","General Appearance","Equipment Related","","","","","Pilot ladder winch lube levelreplenished","2023-12-29T23:59:35","","Completed","2023-12-09T23:59:35","No","No","No","Internal"]
[null,null,null,33414,93785,"106_Thu Jan 11 2024 18:27:49 GMT+0800","2023-11-29T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Side light port and stbd to be de-rusted and painted","Deck - Pipe / Fittings","General Appearance","Equipment Related","","","","","Side light port and stbd  de-rusted and painted","2024-02-29T23:59:35","","Completed","2023-12-18T23:59:35","No","No","No","Internal"]
[null,null,null,33415,95619,"106_Thu Jan 11 2024 18:29:52 GMT+0800","2023-11-29T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Forepeak store door to be de-rusted and painted","Hull & Tanks","General Appearance","Equipment Related","","","","","Forepeak store door de-rusted and painted","2024-02-29T23:59:35","","Completed","2023-12-11T23:59:35","No","No","No","Internal"]
[null,null,null,33416,86312,"106_Thu Jan 11 2024 18:31:46 GMT+0800","2023-11-29T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Steam line on deck forward of 1w cargo tank to be de-rusted and painted","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","Steam line on deck forward of 1w cargo tank de-rusted and painted","2024-02-29T23:59:35","","Completed","2023-12-12T23:59:35","No","No","No","Internal"]
[null,null,null,33417,63299,"106_Thu Jan 11 2024 18:33:10 GMT+0800","2023-11-29T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Funnel deck passage between emergency room and EGCS room to be cleaned of carbon","Accommodation","General Appearance","Equipment Related","","","","","Funnel deck passage between emergency room and EGCS room cleaned of carbon","2023-12-09T23:59:35","","Completed","2023-12-05T23:59:35","No","No","No","Internal"]
[null,null,null,33418,91014,"106_Thu Jan 11 2024 18:34:37 GMT+0800","2023-11-29T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Connection for air/fresh water flushing to be made for Paint store sprinkler system","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","Connection for air/fresh water flushing made for Paint store sprinkler system","2024-02-29T23:59:35","","Completed","2024-01-01T23:59:35","No","No","No","Internal"]
[null,null,null,33419,24724,"106_Thu Jan 11 2024 18:37:25 GMT+0800","2023-11-29T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","CO2 Cabinet near emergency generator room to be de-rusted and painted","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","CO2 Cabinet near emergency generator room de-rusted and painted","2024-01-29T23:59:35","","Completed","2023-12-13T23:59:35","No","No","No","Internal"]
[null,null,null,33420,22483,"106_Thu Jan 11 2024 18:26:07 GMT+0800","2023-11-29T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Gangway lashing D-Shackles to be de-rusted and painted","Deck - Machinery","General Appearance","Equipment Related","","","","","Gangway lashing D-Shackles de-rusted and painted","2024-01-29T23:59:35","","Completed","2024-01-01T23:59:35","No","No","No","Internal"]
[null,null,null,33421,28931,"106_Thu Jan 11 2024 18:23:37 GMT+0800","2023-11-29T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Pilot ladder winch rollers to be de-rusted and painted","Deck - Machinery","General Appearance","Equipment Related","","","","","Pilot ladder winch rollers de-rusted and painted","2024-01-29T23:59:35","","Completed","2023-12-19T23:59:35","No","No","No","Internal"]
[null,null,null,33422,80530,"106_Thu Jan 11 2024 18:40:44 GMT+0800","2023-11-29T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Emergency generator room cooling air exhaust mesh to be cleaned and base to be de-rusted and painted","Miscellaneous","General Appearance","Equipment Related","","","","","Emergency generator room cooling air exhaust mesh cleaned and base to be de-rusted and painted","2024-01-29T23:59:35","","Completed","2023-12-19T23:59:35","No","No","No","Internal"]
[null,null,null,33423,90580,"106_Thu Jan 11 2024 18:42:39 GMT+0800","2023-11-29T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","All vents servicing accommodation/deck/pump room/forepeak store to be inspected by Ship staff Chief Officer and confirm satisfactory opening/closing, cosmetic condition and sealing to prevent ingress/escape of air as required   ","Accommodation,Miscellaneous,Cargo Mach.","Safety / LSA / FFA","Equipment Related","","","","","All vents servicing accommodation/deck/pump room/forepeak store  inspected by Ship staff Chief Officer and confirm satisfactory opening/closing, cosmetic condition and sealing to prevent ingress/escape of air. ","2024-02-29T23:59:35","","Completed","2024-01-01T23:59:35","No","No","No","Internal"]
[null,null,null,33424,61667,"106_Thu Jan 11 2024 18:38:47 GMT+0800","2023-11-29T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Scrubber room door on funnel deck to be de-rusted and painted","Accommodation","General Appearance","Equipment Related","","","","","Scrubber room door on funnel deck de-rusted and painted","2024-01-29T23:59:35","","Completed","2023-12-11T23:59:35","No","No","No","Internal"]
[null,null,null,33425,91848,"106_Thu Jan 11 2024 17:54:04 GMT+0800","2023-11-29T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Safety harness to be put at E/R emergency escape ","LSA / FFA","Eng. / Strg. Comp.","Human Error","","","","","Safety harness  put at E/R emergency escape ","2023-12-06T23:59:35","","Completed","2023-11-30T23:59:35","No","No","No","Internal"]
[null,null,null,33426,95320,"106_Thu Jan 11 2024 18:16:53 GMT+0800","2023-11-29T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Pump room telephone booth packing to be repaired/renewed","Miscellaneous","Safety / LSA / FFA","Equipment Related","","","","","Pump room telephone booth packing  repaired","2023-12-29T23:59:35","","Completed","2023-12-10T23:59:35","No","No","No","Internal"]
[null,null,null,33427,99438,"106_Thu Jan 11 2024 18:18:54 GMT+0800","2023-11-29T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Steam line cascade tank on deck to be de-rusted and painted","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","Steam line cascade tank on deck de-rusted and painted","2024-01-29T23:59:35","","Completed","2023-12-15T23:59:35","No","No","No","Internal"]
[null,null,null,33400,35444,"106_Thu Jan 11 2024 18:19:42 GMT+0800","2023-12-02T23:59:35","Observation","Ship Staff","Ship Staff Insp.","EGCS SW pump change over pressure switch defective, same ordered under BCIA230272","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.31","Very High","","","Pressure switch renewed.","2024-03-17T23:59:35","BCIA230272","Completed","2024-01-20T23:59:35","No","No","No","Internal","13/2 - the order has been delivered onboard; please advise why this is still showing as open. Please update\n\n20/02 - why is this still outstanding - kindly explain; target date moved to 15 March"]
[null,null,null,33401,88451,"106_Thu Jan 11 2024 18:21:29 GMT+0800","2023-12-04T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Fish room defrosting 2 coils observed with low insulation, defective coils need to be replaced with new spare to be received under BCIA240001","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.36","Very High","","","Fish room defective defrosting 2 No. heaters renewed.","2024-04-02T23:59:35","BCIA240001","Completed","2024-04-05T23:59:35","No","No","No","Internal","13/2 -  the subject order has been placed and we await foctry readiness for the same.. Basis vessel's eta to next port, of mid March - target date is extended to MARCH end"]
[null,null,null,33576,83326,"106_Wed Jan 17 2024 16:51:33 GMT+0800","2024-01-11T23:59:35","Defect","Ship Staff","Ship Staff Insp.","IGS Overboard line NRV started leaking through the securing Allen screw. Allen screw removed same was found corroded/wasted.\nAllen screw replaced and putty applied.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","6.12","Medium","","","Leaking valve renewed with new spare.","2024-05-02T23:59:35","BCIA240008","Completed","2024-04-13T23:59:35","No","No","No","Internal","13/2 - spares have been ordered and currently with forwarders. estimating our current ETA of mid march to your next port - target date is being extended by one month. Meanwhile,, closely monitor and advise any deviaiton from normal immediately to office"]
[null,null,null,34190,84079,"106_Wed Feb 14 2024 19:50:41 GMT+0800","2024-02-07T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Nav Audit / Verification","Barometer is found to be sluggish and not giving correct readings","Navigation - Others","Navigation","Equipment Related","4.7","High","","","vessel has ordered for new Barometer, awaiting for supply,\n\nReceived New Barometer on 15th. March. ","2024-05-06T23:59:35","BCIA240012","Completed","2024-03-17T23:59:35","No","No","No","Internal"]
[null,null,null,34191,49210,"106_Wed Feb 14 2024 19:54:36 GMT+0800","2024-02-07T23:59:35","Defect","Ship Staff","Nav Audit / Verification","Two No. GMDSS Walkie - Talkie battery not charging. V/L received PO B CIA230257 with New battery but was found not working.","Navigation - GMDSS & Communication","Communication","Equipment Related","4.27","High","","","vessel has ordered for new GMDSS Walkie talkie Battery awaiting for supply BCIA240011. \nV/L requires 3 Nos batteries as 2 GMDSS radio not charging.\n\nReceived New GMDSS batteries on 14th. March 2024.","2024-05-06T23:59:35","BCIA240011","Completed","2024-03-16T23:59:35","No","No","No","Internal"]
[null,null,null,34982,86143,"0_Mon Mar 25 2024 15:53:02 GMT+0800","2024-03-14T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","IMO symbol for 'Radiation hazard' to be posted","Navigation - GMDSS & Communication","General Appearance","Inappropriate Procedure","","","","","IMO symbol to be posted. \nReceived in Rotterdam and posted. ","2024-05-27T23:59:35","","Completed","2024-05-22T23:59:35","No","No","No","Internal"]
[null,null,null,34988,96898,"0_Sun Apr 07 2024 14:15:46 GMT+0800","2024-03-14T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Forward port side embarkation ladder rope in poor condition","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.47","Medium","","","To order New Embarkation ladder. \nReceived new embarkation ladder at Singapore on 14th. ","2024-05-02T23:59:35","PHAL245013","Completed","2024-03-17T23:59:35","No","No","No","Internal"]
[null,null,null,34989,53828,"106_Mon Mar 25 2024 15:39:04 GMT+0800","2024-03-14T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Cover for electrical junction of provision cranes wasted / corroded","Deck - Machinery","General Appearance","External Factors","","","","","Cover to be fabricated and renewed.\nNew cover fabricated and fitted. ","2024-05-27T23:59:35","","Completed","2024-04-05T23:59:35","No","No","No","Internal"]
[null,null,null,34990,93675,"106_Sun Apr 07 2024 14:06:36 GMT+0800","2024-03-14T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Valves on deck for bunker / COW etc don't have open shut markings","Deck - Pipe / Fittings","Cargo / Ballast Systems","Inappropriate Procedure","","","","","To mark on bunker/COW valves open shut. \nCompleted marking of Open/Shut","2024-05-17T23:59:35","","Completed","2024-04-06T23:59:35","No","No","No","Internal"]
[null,null,null,34991,60724,"0_Mon Mar 25 2024 15:47:39 GMT+0800","2024-03-14T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Christmas tree wire covered with becket. Same to be removed.","Miscellaneous","Structural Condn. / WT integrity ","External Factors","","","","","To remove denso tapes from stay wire, \nRemoved cover on wire","2024-05-27T23:59:35","","Completed","2024-04-08T23:59:35","No","No","No","Internal"]
[null,null,null,34993,75047,"106_Mon Mar 25 2024 15:50:56 GMT+0800","2024-03-14T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Chaffing and wastage in the MF/HF wire connection","Deck - Pipe / Fittings","General Appearance","External Factors","11.8","Low","","","MF-HF wasted shackle and 'U' clamp renewed.","2024-05-27T23:59:35","","Completed","2024-03-28T23:59:35","No","No","No","Internal"]
[null,null,null,34994,94860,"106_Mon Mar 25 2024 15:44:38 GMT+0800","2024-03-14T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Eye wash going to expire in April 2024","Miscellaneous","MLC Related","Inappropriate Procedure","5.46","Medium","","","To replace Expiring Eye wash. \n\nReplaced with New Eye wash received on 14 March24","2024-04-01T23:59:35","BCIA240023","Completed","2024-03-24T23:59:35","No","No","No","Internal"]
[null,null,null,34995,90912,"0_Sun Apr 07 2024 12:06:19 GMT+0800","2024-03-14T23:59:35","Non Conformity,Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","2 Nos. Lifebouys are cracked. ","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.31","High","","","To renew 2 Nos lifebuoys. \nrenewed 2 nos. lifebuoys. ","2024-04-17T23:59:35","","Completed","2024-03-16T23:59:35","No","No","No","Internal"]
[null,null,null,34996,61149,"0_Sun Apr 07 2024 12:10:25 GMT+0800","2024-03-14T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Torches in lifeboat don't have morse signaling capabilities","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.29","High","","","To renew touches and make requisition for morse signaling capable torches,\nReceived on 14th. March completed. ","2024-05-17T23:59:35","BCIA240048","Completed","2024-03-19T23:59:35","No","No","No","Internal"]
[null,null,null,34997,81088,"0_Sun Apr 07 2024 12:03:25 GMT+0800","2024-03-14T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Gap in cement filling upperdeck","Accommodation","Structural Condn. / WT integrity ","External Factors","","","","","To fill Gap of Upper deck cable passage with cement. \nFilled gap of cable passing with cement. ","2024-04-17T23:59:35","","Completed","2024-03-21T23:59:35","No","No","No","Internal"]
[null,null,null,34998,68828,"106_Sun Apr 07 2024 14:11:21 GMT+0800","2024-03-14T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Same colour straps next to each other in Lifeboats. ","LSA / FFA","Safety / LSA / FFA","Inappropriate Procedure","5.28","Very High","","","The Strap in Lifeboatt should be of different colour. \nReplace same colour strap with different colour.","2024-04-17T23:59:35","BCIA240048","Completed","2024-03-18T23:59:35","No","No","No","Internal"]
[null,null,null,34999,12015,"106_Sun Apr 07 2024 12:23:11 GMT+0800","2024-03-14T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","1 nos SCBA set failed to give light and sound alarm at low pressure level","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.43","High","","","To renew SCBA electronic alarm unit.\nRenwed SCBA electronic alarm unit with New. ","2024-04-17T23:59:35","","Completed","2024-03-22T23:59:35","No","No","No","Internal"]
[null,null,null,35000,66730,"106_Sun Apr 07 2024 12:00:33 GMT+0800","2024-03-14T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Hazard of head injury on the ladder going to monkey island","Accommodation","Structural Condn. / WT integrity ","External Factors","11.13","Low","","","To fabricate New hold back hook. \nFabricated New hook for Vent Completed on 29 Mar ","2024-04-19T23:59:35","","Completed","2024-03-31T23:59:35","No","No","No","Internal"]
[null,null,null,35001,22326,"106_Sun Apr 07 2024 12:19:44 GMT+0800","2024-03-14T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Connectors for portable fire extinguishers corroded","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.42","Medium","","","To scrap and paint fire Extinguisher connector. \nScrapped and Painted. ","2024-04-17T23:59:35","","Completed","2024-03-24T23:59:35","No","No","No","Internal"]
[null,null,null,35002,43976,"0_Sun Apr 07 2024 12:13:27 GMT+0800","2024-03-14T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Fire extinguishers colour coding size not as required by C.O.S.W.P","LSA / FFA","Safety / LSA / FFA","Inappropriate Procedure","5.42","Medium","","","To colour code fire extinguishers as per C.O.S.W.P\nOne of the the extinguisher was not colour coded same corrected.  ","2024-04-17T23:59:35","","Completed","2024-03-27T23:59:35","No","No","No","Internal"]
[null,null,null,35822,26329,"106_Sat Jun 01 2024 17:31:46 GMT+0800","2024-03-14T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Lifeboat gripe wire in poor condition. Secured with only 2 bulldog grip","LSA / FFA","Safety / LSA / FFA","Human Error","5.28","Very High","","","To place one more Bull dog grip on the wire. \nPlaced one more extra grip on the wire","2024-06-01T23:59:35","PHAL240007","Completed","2024-03-31T23:59:35","No","No","No","Internal"]
[null,null,null,35823,54946,"106_Sat Jun 01 2024 17:36:23 GMT+0800","2024-03-14T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Tripping hazards in pump room to be highlighted","Miscellaneous","Cargo / Ballast Systems","External Factors","","","","","Tripping hazard to be highlighted in P/R. \nTripping hazards in pump room marked and highlighted","2024-05-02T23:59:35","","Completed","2024-04-14T23:59:35","No","No","No","Internal"]
[null,null,null,35824,72539,"106_Sat Jun 01 2024 17:40:38 GMT+0800","2024-03-14T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Chipping gun secured with cable tie in on position. Air hose is damaged","Deck - Machinery","Crew Management","Human Error,Inappropriate Procedure","","","","","Chipping gun secured with cable tie in on position. Air hose is damaged\nRemoved securing arrangement for Chipping Gun and replaced Air hose. ","2024-04-01T23:59:35","","Completed","2024-03-15T23:59:35","No","No","No","Internal"]
[null,null,null,35826,53690,"106_Sat Jun 01 2024 19:46:48 GMT+0800","2024-03-14T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Tell tale sign of minor leakage from L.O cooler","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.3","Medium","","","Lub oil leakage was identified as Defective pressure gauge,same renewed","2024-04-14T23:59:35","","Completed","2024-03-18T23:59:35","No","No","No","Internal"]
[null,null,null,35827,45591,"106_Sat Jun 01 2024 19:50:59 GMT+0800","2024-03-14T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Lights in Forepeak not operational","Elect. Mach. & Equip.","General Appearance","External Factors","","","","","Fused bulbs replaced with new.","2024-03-22T23:59:35","","Completed","2024-03-17T23:59:35","No","No","No","Internal"]
[null,null,null,35828,21938,"106_Sat Jun 01 2024 20:17:34 GMT+0800","2024-03-14T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Yellow circle below fire detector ","Miscellaneous","General Appearance","Human Error","","","","","detector number painted within yellow circle","2024-03-24T23:59:35","","Completed","2024-03-17T23:59:35","No","No","No","Internal"]
[null,null,null,35830,21416,"106_Sat Jun 01 2024 20:04:12 GMT+0800","2024-03-14T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Cable penetration for COP/ballast pump sensor is out","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","Sensor cable outer sheathing renewed","2024-04-14T23:59:35","","Completed","2024-03-30T23:59:35","No","No","No","Internal"]
[null,null,null,35831,40641,"106_Sat Jun 01 2024 20:47:12 GMT+0800","2024-03-14T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Tell tale signs of minor leakages","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Seepage at Flanges rectified by tightening/renewal of gaskets.Presure gauge fittings nipped up at pumps to rectify minor weeping","2024-05-14T23:59:35","","Completed","2024-04-17T23:59:35","No","No","No","Internal"]
[null,null,null,35832,40503,"106_Sat Jun 01 2024 20:35:59 GMT+0800","2024-03-14T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Light in Em Escape  from ER is unlit","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Human Error","","","","","Fused bulb renewed","2024-03-19T23:59:35","","Completed","2024-03-15T23:59:35","No","No","No","Internal"]
[null,null,null,35833,74117,"106_Sat Jun 01 2024 20:08:02 GMT+0800","2024-03-14T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Carbon deposits below ODME pump coupling in Pump room","Deck - Machinery","Cargo / Ballast Systems","Equipment Related","","","","","Coupling inspected and  one bolt found slightly slack,same tightened ","2024-05-03T23:59:35","","Completed","2024-04-12T23:59:35","No","No","No","Internal"]
[null,null,null,35834,19430,"106_Sat Jun 01 2024 20:39:01 GMT+0800","2024-03-14T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Alkaline/Acid/Neutral stored in a single rack","Miscellaneous","Eng. / Strg. Comp.","Knowledge Based","","","","","Chemical drums segregated and arranged seperately ","2024-03-28T23:59:35","","Completed","2024-03-20T23:59:35","No","No","No","Internal"]
[null,null,null,35835,68312,"106_Sat Jun 01 2024 20:52:25 GMT+0800","2024-03-14T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Section of Antiskid missing in SG Room","Miscellaneous","Eng. / Strg. Comp.","Human Error","","","","","Antiskid applied at missing area.","2024-03-24T23:59:35","","Completed","2024-03-23T23:59:35","No","No","No","Internal"]
[null,null,null,34983,85432,"106_Fri Apr 05 2024 19:24:04 GMT+0800","2024-03-20T23:59:35","Defect","Ship Staff","Ship Staff Insp.","No.2 Steering Gear starter panel low speed mode phase monitor (phase fail relay) defective.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.3","Medium","","","No.2 Steering Gear starter panel low speed mode phase monitor need to be renewed. RO - PHAL240005 raised.Spare received on board. Relay renewed and system working satisfactory.","2024-10-01T23:59:35","PHAL240005","Completed","2024-08-25T23:59:35","No","No","No","Internal"]
[null,null,null,34986,44613,"106_Sat Apr 06 2024 13:40:57 GMT+0800","2024-03-22T23:59:35","Defect","Ship Staff","Ship Staff Insp.","BWTS valve PV202 positioner faulty. ","E/R - Aux. Mach.","Cargo / Ballast Systems","Equipment Related","10.31","Very High","","","BWTS valve PV202 defective positioner need to renew. Ro - PHAL240009 raised.\nCommunication with office in progress, power supply card checked.\nNew SIPART controller received and fitted,tested,satisfactory","2024-09-07T23:59:35","PHAL240009","Completed","2024-08-16T23:59:35","No","No","No","Internal"]
[null,null,null,35655,56699,"106_Thu May 30 2024 20:34:47 GMT+0800","2024-03-25T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","COT inspection to be carried out as vessel is tank cleaning and making entry in COT","Hull & Tanks","Cargo / Ballast Systems","Industry Issue","2.9","Medium","","","To carry out tank inspection and make reports.\nCompleted on 1st. April after tank cleaning operations. ","2024-04-17T23:59:35","","Completed","2024-04-03T23:59:35","No","No","No","Internal"]
[null,null,null,35656,60193,"106_Thu May 30 2024 20:43:13 GMT+0800","2024-03-25T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Port side deck store to be organized","Deck - Machinery","General Appearance","Inappropriate Procedure","","","","","To Organize Port side deck store. \nCompleted ","2024-04-26T23:59:35","","Completed","2024-04-23T23:59:35","No","No","No","Internal"]
[null,null,null,35657,76932,"106_Thu May 30 2024 20:45:32 GMT+0800","2024-03-25T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Cargo tank domes need to be derusted and painted. ","Deck - Pipe / Fittings","General Appearance","External Factors","","","","","Cargo tank domes need to be derusted and painted. \nCompleted derusting of tank domes","2024-05-26T23:59:35","","Completed","2024-05-24T23:59:35","No","No","No","Internal"]
[null,null,null,35658,44913,"106_Thu May 30 2024 20:38:25 GMT+0800","2024-03-25T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","SEP Annex 1 procedures to be promulgated and corrected for New ship’s Name","Documentation","Cert. & Docu.","Inappropriate Procedure","2.3","High","","","To Correct for New ships Name. \nCorrected with New Ships Name. ","2024-04-06T23:59:35","","Completed","2024-03-27T23:59:35","No","No","No","Internal"]
[null,null,null,35659,54039,"106_Thu May 30 2024 20:48:29 GMT+0800","2024-03-25T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Gangway wires (P/S) needs to be greased","Deck - Machinery","Safety / LSA / FFA","Inappropriate Procedure","5.47","Medium","","","To Grease Gangway wires (P/S). \nCompleted greased Gangway wires port and stbd. ","2024-04-26T23:59:35","","Completed","2024-04-06T23:59:35","No","No","No","Internal"]
[null,null,null,35660,67588,"106_Thu May 30 2024 22:45:36 GMT+0800","2024-03-25T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","COPT Platform Steam U clamp found Loose.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","External Factors","11.5","Medium","","","U clamp tightened and double nut fitted to avoid loosening.","2024-04-04T23:59:35","","Completed","2024-04-01T23:59:35","No","No","No","Internal"]
[null,null,null,35661,51742,"106_Thu May 30 2024 22:08:01 GMT+0800","2024-03-25T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Small section of Walkway in Steering gear room observed without Antiskid Paint.","Miscellaneous","Eng. / Strg. Comp.","Human Error","10.43","Medium","","","Antiskid Paint applied at missing area.","2024-03-24T23:59:35","","Completed","2024-03-20T23:59:35","No","No","No","Internal"]
[null,null,null,35662,76023,"106_Thu May 30 2024 22:04:42 GMT+0800","2024-03-25T23:59:35","Other,Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Drums in Steering Gear Room found lashed with smaller Dia wire","Miscellaneous","Eng. / Strg. Comp.","Human Error","10.42","Medium","","","Lashing wire replaced with thicker wire","2024-03-24T23:59:35","","Completed","2024-03-19T23:59:35","No","No","No","Internal"]
[null,null,null,35663,47996,"106_Thu May 30 2024 22:49:29 GMT+0800","2024-03-25T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Main Engine Exhaust Pipe Lagging on Reactor valve found damaged","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Human Error","10.19","Very High","","","Damaged Lagging Renewed.","2024-03-28T23:59:35","","Completed","2024-03-27T23:59:35","No","No","No","Internal"]
[null,null,null,35664,82751,"106_Thu May 30 2024 22:43:00 GMT+0800","2024-03-25T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Aux Engine Fuel Circ Pump Discharge Pressure gauge showing erratic readings","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Pressure gauge renewed and checked with stby pump,satisfactory","2024-04-01T23:59:35","","Completed","2024-05-28T23:59:35","No","No","No","Internal"]
[null,null,null,35665,41676,"106_Thu May 30 2024 22:34:35 GMT+0800","2024-03-25T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Em DG Room Vent flaps were found hard to operate","LSA / FFA","Safety / LSA / FFA","External Factors","5.40","Very High","","","Vent flaps for Em Dg room eased up and lubricated.Operation satisfactory.","2024-04-02T23:59:35","","Completed","2024-03-30T23:59:35","No","No","No","Internal"]
[null,null,null,35666,40222,"106_Thu May 30 2024 22:19:08 GMT+0800","2024-03-25T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Safety Googles on Workshop machinery found dirty","Miscellaneous","Eng. / Strg. Comp.","Human Error","10.29","Medium","","","All Safety glasses cleaned.","2024-03-24T23:59:35","","Completed","2024-03-19T23:59:35","No","No","No","Internal"]
[null,null,null,35667,17240,"106_Thu May 30 2024 20:41:01 GMT+0800","2024-03-25T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Manhole covers for WBT and COT to be de-rusted and painted after inspection of COT and WBT is completed.  ","Hull & Tanks","General Appearance","External Factors","","","","","Manhole covers for WBT and COT to be de-rusted and painted Completed Derusting and painting of cargo tanks and WBT.  ","2024-05-24T23:59:35","","Completed","2024-05-23T23:59:35","No","No","No","Internal"]
[null,null,null,35668,57239,"106_Thu May 30 2024 22:22:50 GMT+0800","2024-03-25T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Spare Exhaust Valves removed from Main Engine Units to be overhauled and kept ready for use.","E/R - Main Engine","Eng. / Strg. Comp.","Equipment Related,External Factors","10.32","Very High","","","Spare Exhaust valve overhauled,tested and kept ready for use","2024-04-19T23:59:35","","Completed","2024-03-25T23:59:35","No","No","No","Internal"]
[null,null,null,35693,null,"106_Sat Jun 01 2024 06:01:16 GMT+0000","2024-03-25T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Oil noted near COPT #3, same to be rectified","Deck - Machinery","Cargo / Ballast Systems","Equipment Related","","","","","Checked found no leakages from seal, oil dropped from grease & same cleaned","2024-06-01T23:59:35","","Completed","2024-05-02T23:59:35","No","No","No","Internal"]
[null,null,null,34992,18037,"106_Sun Apr 07 2024 17:16:01 GMT+0800","2024-03-25T23:59:35","Observation","Ship Staff","Ship Staff Insp.","Cargo sea chest valve COV069 observed not holding, suspecting damaged seat ring.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","10.31","Very High","","","Valve seat ring or complete valve to be renewed at Dry Dock, same included in Dry Dock specs, Line is now blanked with spectacle blank.","2025-03-01T23:59:35","PHAL240023 for seat rings and PHAL240017 for complete valve.","Completed","2024-10-17T23:59:35","No","No","No","Internal"]
[null,null,null,34987,89351,"106_Fri Apr 05 2024 19:28:44 GMT+0800","2024-03-26T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Incinerator dilution damper pneumatic cylinder solenoid valve defective.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.3","Medium","","","Incinerator dilution damper pneumatic cylinder defective solenoid valve need to be renewed. RO - PHAL240012 raised.New solenoid received and fitted,working satisfactory","2024-09-06T23:59:35","PHAL240012","Completed","2024-08-13T23:59:35","No","No","No","Internal"]
[null,null,null,34985,82761,"106_Fri Apr 05 2024 19:38:38 GMT+0800","2024-04-04T23:59:35","Defect","Ship Staff","Ship Staff Insp.","IGS Deck Seal pump No.1 impeller found 60% wasted and not building enough pressure.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.35","Very High","","","IGS Deck Seal pump No.1 need to be overhauled. RO - PHAL240018 raised. Spares received.Pump overhauled.New impeller and shaft sleeve and seal fitted,satisfactory","2024-09-01T23:59:35","PHAL240018","Completed","2024-09-12T23:59:35","No","No","No","Internal"]
[null,null,null,34984,82692,"106_Fri Apr 05 2024 19:34:33 GMT+0800","2024-04-05T23:59:35","Defect","Ship Staff","Ship Staff Insp.","AE FO pressure transmitters malfunctioning.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.3","Medium","","","AE FO defective pressure transmitters need to be renewed. RO - PHAL240022 raised.New transmitters received and installed.Pressure transmitters working satisfactory.","2024-07-02T23:59:35","PHAL240022","Completed","2024-06-12T23:59:35","No","No","No","Internal"]
[null,null,null,35109,78935,"106_Tue May 07 2024 15:22:34 GMT+0800","2024-04-11T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Calorifier temperature controller defective","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.19","Very High","","","PHAL240024 has been raised for required spare, same to be replaced upon receipt. Spare received.Installed and setting adjusted as received from Supt.Working satisfactory","2024-08-30T23:59:35","PHAL240024","Completed","2024-09-07T23:59:35","No","No","No","Internal"]
[null,null,null,33399,18917,"106_Thu Jan 11 2024 18:29:24 GMT+0800","2024-04-20T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Please note 440V low insulation was traced from 2 heating elements in the baking oven. There are no spare coils onboard, vessel has raised BCIA240002 for spare heating elements.","Accommodation","General Appearance","Equipment Related","10.35","Very High","","","New heating elements  were received and damaged elements were replaced. Baking Oven is operating normal now, with out low insulation.","2024-12-21T23:59:35","PHAL240092","Completed","2024-10-29T23:59:35","No","No","No","Internal","13/2 - the PO is under process. basis your next port ETA of Mid March, target date is being extended by one month."]
[null,null,null,33398,10389,"106_Thu Jan 11 2024 18:24:12 GMT+0800","2024-04-26T23:59:35","Observation","Ship Staff","Ship Staff Insp.","EGCS AE scrubber quencher valve 36 solenoid coil found malfunctioning, to make it operational coil from Aux Boiler 27-2 was consumed., vessel has raised BCIA240003 for spare coils.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.31","Very High","","","Solenoid coil to be replaced upon receipt of new spare.\nNew coil received and installed,working satisfactory.","2024-09-01T23:59:35","PHAL240045","Completed","2024-08-09T23:59:35","No","No","No","Internal","13/2 - order is under process. basis vessel's eta to next port, of mid March - target date is extended by 1 month."]
[null,null,null,35111,80854,"106_Tue May 07 2024 15:17:10 GMT+0800","2024-04-28T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Clean bilge 15ppm monitor displaying \" Battery replacement\"  error. Battery needs to be replaced.","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.11","Medium","","","New spare battery received and installed and fault cleared.","2024-06-02T23:59:35","PHAL240047","Completed","2024-05-25T23:59:35","No","No","No","Internal"]
[null,null,null,33397,31857,"106_Thu Jan 11 2024 18:27:21 GMT+0800","2024-05-02T23:59:35","Observation,Breakdown","Ship Staff","Ship Staff Insp.","Crew laundry room exhaust fan found vibrating and accompanied by abnormal sound. Exhaust fan was removed from place for investigation, upon which found bearings and motor damaged with rubbing marks on the windings. \nIn view of the above BCIA230276 VENTILATION: CREW LAUNDRY EXH FAN has been raised.","Accommodation","General Appearance","Equipment Related","10.31","Very High","","","Vent fan to be replaced upon receipt of spare. Spare received.Installed and tested,satisfactory","2024-09-01T23:59:35","\tPHAL240044","Completed","2024-08-29T23:59:35","No","No","No","Internal","13/2 - 13/2 - order is under process. basis vessel's eta to next port, of mid March - target date is extended by 1 month. trust temporary arrangements have been done."]
[null,null,null,34189,40194,"106_Tue Feb 13 2024 18:37:10 GMT+0800","2024-05-02T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","Service air compressor cooler noted leaking, repairs attempted by still leak persists.","E/R - Air Comp.","Eng. / Strg. Comp.","Equipment Related","10.30","High","","","Communication with makers in progress for spare cooler.Spare cooler received.Spare new cooler received and installed in place.Tested and found working satisfactory.","2024-10-01T23:59:35","","Completed","2024-08-21T23:59:35","No","No","No","Internal","20/02 - maker replaceing the same vide GC. will be deliveed onboard soonest."]
[null,null,null,35110,70188,"106_Tue May 07 2024 15:26:30 GMT+0800","2024-05-05T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Both LT coolers SW eccentric reducer developed hole due to corrosion. Leaks arrested by carrying out cold work repairs","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.1","Medium","","","PHAL240026 has been raised for required material. For permanent repairs to be carried out, pipe sections have to be removed at 3 connection flanges and 2 bolted padding. Due to the above mention piping arrangement, permanent repairs present as a difficult job needing sufficient time to prepare for jig, skilled welding and alignment etc.Spare flanges received ,awaiting suitable oppurtunity to carry out the job.Inlet pipe for No.1 cooler reducer renewed. All four reducers renewed.Outlet pipe reducer fitted with flange at both sides.","2024-09-02T23:59:35","PHAL240026","Completed","2024-09-07T23:59:35","No","No","No","Internal"]
[null,null,null,35108,48119,"106_Tue May 07 2024 15:20:35 GMT+0800","2024-05-09T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Fixed gas detection system #1 sampling for ballast tanks solenoids defective. ","Elect. Mach. & Equip.","Cargo / Ballast Systems","Equipment Related","5.1","Very High","","","PHAL240030 has been raised for required solenoid valves.Spare Solenoid received and fitted.Sample Pipes removed and blown through.System connect back and running satisfactory,under observation.","2024-07-17T23:59:35","PHAL240030.","Completed","2024-06-16T23:59:35","No","No","No","Internal"]
[null,null,null,35107,93789,"106_Tue May 07 2024 15:14:20 GMT+0800","2024-05-12T23:59:35","Breakdown","Ship Staff","Ship Staff Insp.","FWG flowmeter defective","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.15","Low","","","Defective flowmeter to be renewed, PHAL240046 has been raised for spare flowmeter.Spare flowmeter received and installed,working satisfactory.","2024-09-01T23:59:35","PHAL240046","Completed","2024-08-14T23:59:35","No","No","No","Internal"]
[null,null,null,36548,84679,"0_Tue Jul 16 2024 09:41:34 GMT+0800","2024-06-08T23:59:35","Observation,Defect","Ship Staff","Ship Staff Insp.","Main Eng Fuel Circ Pump No.2 Seal leaks after changeover to LSMGO.Drive shaft bearing loose in casing.","E/R - Pumps","Eng. / Strg. Comp.","Equipment Related,Industry Issue","10.31","Very High","","","Pump opened up and seal renewed. Tested, satisfactory, No leaks. However found the shaft worn down in area of bearing. Spare requested and received at Singapore. ","2024-12-21T23:59:35","PHAL240071","Completed","2024-09-06T23:59:35","No","No","No","Internal"]
[null,null,null,36549,50586,"106_Tue Jul 16 2024 08:13:51 GMT+0800","2024-06-30T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Fwd Hyd Oil System Oil sample showing Caution for water content","Deck - Machinery","Mooring","External Factors","","","","","Checked and confirmed that the Vent pipe for storage tank is not wasted and pressure testing of LO cooler was carried out and no leaks found.. So it was confirmed that the source of water contamination was condensation. Filtration unit was requested and received at Singapore. During sailing the system oil was transferred in to storage tank and heated and filtered and drained to remove water. After the  filtration the water content was observed to be <0.02 % . Fresh sample was landed for testing and the result is \"NORMAL\". Recommend to carry out filtration, when ever vessel is having long voyages, to remove condensation water from system, so that condensate shall not accumulate.","2025-03-01T23:59:35","PHAL245101","Completed","2025-01-05T23:59:35","No","No","No","Internal"]
[null,null,null,36551,36644,"106_Tue Jul 16 2024 09:38:04 GMT+0800","2024-07-09T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Shaft earthing Device records higher voltage than normal\n","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.31","Very High","","","Split rings cleaned, shaft surface cleaned and split rings were inverted. After assembling back, the voltage was observed to be with in limits. System observed after sailing out and till now voltage is in the range of 12 ~ 16 mV.","2025-02-21T23:59:35","PHAL240107","Completed","2024-11-01T23:59:35","No","No","No","Internal"]
[null,null,null,36993,94114,"106_Thu Aug 01 2024 14:03:49 GMT+0800","2024-07-17T23:59:35","Defect","Ship Staff","Ship Staff Insp.","LT cooling expansion tank show sheen of Lub oil on top of water  surface.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Source of contamination identified as from No.3 A/E LO cooler. Cooler 0-rings were renewed and leak has been rectified.  After few days of collecting and removing oil from top of expansion tank water, chemical was added to remove the oil and at next opportunity the system water shall be drained and replaced with fresh water.. O-rings of remaining two coolers were also renewed.","2025-03-31T23:59:35","","Completed","2025-01-04T23:59:35","No","No","No","Internal"]
[null,null,null,36990,77754,"106_Thu Aug 01 2024 14:47:15 GMT+0800","2024-07-23T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Sampling Pump for gas detection system (WBT) is noisy","Elect. Mach. & Equip.","Cargo / Ballast Systems","Equipment Related","8.46","Very High","","","Diaphrgm renewed and tested, still pump is noisy. Suspect the motor bearing is defective. Spare pump requested and received at Le Havre and replaced. System now operating normally.","2024-10-31T23:59:35","PHAL240117","Completed","2024-10-03T23:59:35","No","No","No","Internal"]
[null,null,null,37423,40063,"0_Wed Sep 18 2024 18:55:47 GMT+0800","2024-07-26T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Control Air compressor Auto drain malfunctioned","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.31","Very High","","","Spare requested and received at Le Havre. Auto drain unit was renewed and put back in use.","2024-10-24T23:59:35","PHAl240109","Completed","2024-09-29T23:59:35","No","No","No","Internal"]
[null,null,null,37019,65839,"106_Thu Aug 01 2024 14:41:54 GMT+0800","2024-07-30T23:59:35","Defect","Ship Staff","Ship Staff Insp.","EGCS Wash water analyser display show blank without any sensor readings and shipstaff unable to access the menu","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","10.32","Very High","","","Awaiting Maker's advice to resolve the issue.Received Maker advice and rectified the fault.Display showing normal.","2024-08-31T23:59:35","","Completed","2024-08-14T23:59:35","No","No","No","Internal"]
[null,null,null,37422,92884,"106_Wed Sep 18 2024 18:53:15 GMT+0800","2024-07-31T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Control air dryer defective and tripped on High temperature","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","10.31","Very High","","","Tried charging gas  but unsuccessful. Also Dryer electrical components are defective. New drier ordered and received at Singapore and installed. Drier was put in to use and is now operational.","2025-03-01T23:59:35","PHAL240131 AND 240133","Completed","2024-12-14T23:59:35","No","No","No","Internal"]
[null,null,null,36986,11481,"106_Thu Aug 01 2024 14:49:38 GMT+0800","2024-07-31T23:59:35","Defect","Ship Staff","Ship Staff Insp.","EGCS-Aux Engine Scrubber Gas outlet temperature showing erratic values","E/R - Pipes/ valves & fittings,Elect. Mach. & Equip.","Eng. / Strg. Comp.","Equipment Related","","","","","SENSOR CLEANED STILL THE VALUES ARE ERRATIC, Spare sensor ordered and received at Singapore and was renewed. The defect is now closed.","2025-03-01T23:59:35","PHAL240122","Completed","2024-12-04T23:59:35","No","No","No","Internal"]
[null,null,null,36987,22661,"106_Mon Aug 19 2024 15:47:15 GMT+0800","2024-08-10T23:59:35","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Decontamination shower in engine room 2nd platform not ready. Decontamination shower valves in poop deck are not free.","Miscellaneous","Eng. / Strg. Comp.","Human Error","","","","","Decontamination shower on 2nd platform rectified, wires put back.\nShower is now operational. ","2024-08-31T23:59:35","","Completed","2024-08-21T23:59:35","No","No","No","Internal"]
[null,null,null,36988,18179,"106_Mon Aug 19 2024 15:49:44 GMT+0800","2024-08-10T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","VRCS Return filter Showing RED,indicating dirty","Deck - Pipe / Fittings","Eng. / Strg. Comp.","Equipment Related","","","","","Spare requested and received on board.Spare filter installed and the indication is normal","2024-09-27T23:59:35","","Completed","2024-09-19T23:59:35","No","No","No","Internal"]
[null,null,null,36989,32865,"0_Mon Aug 19 2024 15:53:41 GMT+0800","2024-08-10T23:59:35","Critical Equipment,Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Fixed CO2 for Emergency Generator room - Manual release elvers could not be removed from location. Fixed CO2 for Emergency Generator room - box hinges need maintenance. Fixed CO2 for Emergency Generator room - Valves needs maintenance\n","Critical Equip.","Safety / LSA / FFA","Equipment Related","","","","","To inspect and rectify.Co 2 room discharge valve eased up.Manual operating pins cleaned and coated with light grease.Box hinge greased","2024-10-02T23:59:35","","Completed","2024-09-06T23:59:35","No","No","No","Internal"]
[null,null,null,36991,18711,"0_Mon Aug 19 2024 15:55:32 GMT+0800","2024-08-10T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ESB 220v LOW INSULATION","Elect. Mach. & Equip.","Eng. / Strg. Comp.","External Factors","","","","","To inspect and rectify.Port side Embarkation light was having Moisture ingress.Same cleaned up and checkd seal,satisfactory.Now Insulation is above 5MOhms.","2024-08-31T23:59:35","","Completed","2024-08-21T23:59:35","No","No","No","Internal"]
[null,null,null,36992,74632,"106_Mon Aug 19 2024 15:44:37 GMT+0800","2024-08-10T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Various Leaks observed in Engine room.\n1.Oil Mist spray near SCR throttle valve.\n2.AE Fuel supply PP leak observed at changeover valve.\n3.No.3 DG Centrifuge filter","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.31","Very High","","","Spares Have been requested for Supply Pump changeover valve and DG Centrifuge filter and were received at Singapore. The centrifugal filter was renewed and now no leaks. The supply pump change over valve was removed and o-rings were renewed and now there is no leak.","2025-03-01T23:59:35","For Item No.2 & No.3PHAL240135 & 136 are in place","Completed","2024-12-17T23:59:35","No","No","No","Internal"]
[null,null,null,36994,84884,"106_Mon Aug 19 2024 16:06:52 GMT+0800","2024-08-10T23:59:35","Defect","Ship Staff","Suptd. Insp.","ER workshop grinder not operational","E/R - Aux. Mach.","Eng. / Strg. Comp.","Equipment Related","","","","","Spare ordered.Received and installed,tested,satisfactory","2024-10-16T23:59:35","PHAL 240121","Completed","2024-10-03T23:59:35","No","No","No","Internal"]
[null,null,null,36995,96591,"0_Mon Aug 19 2024 19:03:27 GMT+0800","2024-08-10T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","The forward mast and mast riser stay wires are rusted heavily.","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","Equipment Related","","","","","De-rusted and greased","2024-10-15T23:59:35","","Completed","2024-09-19T23:59:35","No","No","No","Internal"]
[null,null,null,36996,67932,"106_Mon Aug 19 2024 19:09:04 GMT+0800","2024-08-10T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","COW machine valve indicators are faded or painted over. Lashing ropes missing","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","De-rusted and painted, lashing rope put","2024-09-10T23:59:35","","Completed","2024-09-01T23:59:35","No","No","No","Internal"]
[null,null,null,36997,61988,"0_Mon Aug 19 2024 19:02:05 GMT+0800","2024-08-10T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Water inside the Midship locker Port side Ex-rated light indicating seals are damaged     ","Elect. Mach. & Equip.","General Appearance","External Factors","","","","","To inspect and rectify.Complete lamp fitting received at Singapore fitted in place and tested,satisfactory","2024-08-31T23:59:35","","Completed","2024-08-22T23:59:35","No","No","No","Internal"]
[null,null,null,36998,61868,"106_Mon Aug 19 2024 18:58:23 GMT+0800","2024-08-10T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Many of the U clamps on the main deck are rusted. Clamps of valve hydraulic pipelines are rusted and wasted. Needs immediate attention. Engine room to slop tank spool rusted heavily. A few valves and connections forward of the pumproom area need maintenance     ","Deck - Pipe / Fittings","General Appearance","Industry Issue","","","","","Descaling and coating carried out.","2024-12-21T23:59:35","","Completed","2024-11-14T23:59:35","No","No","No","Internal"]
[null,null,null,36999,50452,"0_Mon Aug 19 2024 19:09:55 GMT+0800","2024-08-10T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Pilot ladder securing ropes - strands are open. Crack in Port side pilot ladder. Pilot ladder reel winches are rusted. Nut bolts are wasted. Stbd side pilot ladder rope needs urgent attention. Stbd side accommodation ladder - is tiled to one side when used. Railing in bend. Gangway operating levers not coming to neutral position by itself Embarkation ladder in forward - thimble rusted. Rope is covered with canvas. If the rope is wet, the canvas will prevent the rope from drying.     ","Miscellaneous","General Appearance","Industry Issue","","","","","Port side pilot ladder renewed with spare ladder. De-rusting and painting of pilot ladder winches carried out. Accommodation ladder maintenance included in DD specs,  Gangway hoisting system overhauled, Embarkation ladder forward canvas removed and thimble de-rusted. ","2024-09-10T23:59:35","","Completed","2024-09-10T23:59:35","No","No","No","Internal"]
[null,null,null,37000,28168,"0_Mon Aug 19 2024 19:12:29 GMT+0800","2024-08-10T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Portable foam applicator in Emergency Generator room - Quick coupling is jammed. The suction hose cannot be connected. Masking tape in the many fire hoses     ","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","inspected and freed","2024-08-31T23:59:35","","Completed","2024-08-18T23:59:35","No","No","No","Internal"]
[null,null,null,37001,56990,"0_Mon Aug 19 2024 19:14:12 GMT+0800","2024-08-10T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Bridge wing telegraph controls - showing 5% & 7% when engine is stopped. ALDIS lamp socket in monkey island cannot be opened","Elect. Mach. & Equip.","Eng. / Strg. Comp.","Industry Issue","","","","","ALDIS lamp socket freed and can be opened now.\nBridge wing telegraph controls adjusted, Confirmed operation from all locations.","2024-12-01T23:59:35","","Completed","2024-10-25T23:59:35","No","No","No","Internal"]
[null,null,null,37002,75798,"106_Mon Aug 19 2024 19:14:23 GMT+0800","2024-08-10T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Steam manifold valves are not moving. A few caps missing from the cargo tank steam coils are missing. There are no records or signs of maintenance in the cargo tank steam heating coil steam traps. One of the steam supply valves in the Engine room is leaking.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","Valves overhauled and freed. Cocks to be put on steam trap drains. E/R Valve will have to be overhauled in coming drydock and has been added in the DD Spec. ","2025-03-01T23:59:35","","Completed","2024-12-28T23:59:35","No","No","No","Internal"]
[null,null,null,37003,23475,"0_Mon Aug 19 2024 19:17:19 GMT+0800","2024-08-10T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","MOB marker rope length is short. MOB marker lifebuoy showing crack signs     ","","Safety / LSA / FFA","Industry Issue","","","","","Rope changed, RO raised for a new MOB lifebuoy, and received at Le Havre.","2024-10-16T23:59:35","PHAL240143","Completed","2024-09-29T23:59:35","No","No","No","Internal"]
[null,null,null,37004,64396,"106_Mon Aug 19 2024 19:18:42 GMT+0800","2024-08-10T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Bunker manifold nut bolts are wasted. Spare reducers are rusted and need immediate attention. Spare vapor manifold reducers do not have studs at 12 O Clock position","Deck - Pipe / Fittings","General Appearance","Equipment Related","","","","","Reducers de-rusted and painted. Bunker manifold de-rusted and painted. Stud fixed at 12 o clock","2024-09-20T23:59:35","","Completed","2024-09-08T23:59:35","No","No","No","Internal"]
[null,null,null,37005,64189,"0_Mon Aug 19 2024 19:19:20 GMT+0800","2024-08-10T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Elevator trunk escape way hatches are not free.     ","Miscellaneous","General Appearance","Industry Issue","","","","","All the elevator shaft  hatches inspected, lubricated and freed","2024-08-31T23:59:35","","Completed","2024-08-31T23:59:35","No","No","No","Internal"]
[null,null,null,37006,63300,"106_Mon Aug 19 2024 19:20:21 GMT+0800","2024-08-10T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","ODME valves are getting rusted and have delicate parts. Immediate attention is required.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","Valves are de-rusted and painted","2024-09-20T23:59:35","","Completed","2024-09-01T23:59:35","No","No","No","Internal"]
[null,null,null,37007,44459,"0_Mon Aug 19 2024 19:22:34 GMT+0800","2024-08-10T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","The pressure regulator was not fitted to the cargo sea chest testing arrangement in the pumproom to limit test pressure to 3.0 Bars","Deck - Machinery,Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","Pressure regulator fitted and arrangement made for testing.","2025-03-01T23:59:35","","Completed","2024-11-19T23:59:35","No","No","No","Internal"]
[null,null,null,37008,61367,"0_Mon Aug 19 2024 19:26:20 GMT+0800","2024-08-10T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Few valves in the foam room are at high and cannot be operated by a person with average height. Suggest making a platform","Deck - Pipe / Fittings","Structural Condn. / WT integrity ","Industry Issue","","","","","Platform fabricated for the same","2024-10-10T23:59:35","","Completed","2024-09-16T23:59:35","No","No","No","Internal"]
[null,null,null,37009,35413,"0_Mon Aug 19 2024 19:28:06 GMT+0800","2024-08-10T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Ballast Gas sampling system - The transportation pump was kept bypassed.","Miscellaneous","Cargo / Ballast Systems","Behaviour Based","","","","","Training carried out, the gas sampling point should be disabled one by one and not as one complete unit.","2024-09-24T23:59:35","","Completed","2024-08-19T23:59:35","No","No","No","Internal"]
[null,null,null,37010,84886,"0_Mon Aug 19 2024 19:28:39 GMT+0800","2024-08-10T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","No 2-cargo manifold pressure gauge point is leaking in port side manifold","Deck - Pipe / Fittings","General Appearance","External Factors","","","","","tightened, cleaned and tested","2024-09-10T23:59:35","","Completed","2024-09-10T23:59:35","No","No","No","Internal"]
[null,null,null,37011,23466,"106_Mon Aug 19 2024 19:29:40 GMT+0800","2024-08-10T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Load line marks are faded and need remarking.","Hull & Tanks","Structural Condn. / WT integrity ","Equipment Related","","","","","During drifting at sea vessel repainted the Port side load line marks.\nStbd side load line checked and found in good order.","2025-03-01T23:59:35","","Completed","2025-02-06T23:59:35","No","No","No","Internal"]
[null,null,null,37012,96686,"0_Mon Aug 19 2024 19:24:08 GMT+0800","2024-08-10T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Lifeboat/rescue boat instructions are faded. Board oars not marked with ship name. Port side lifeboat forward glass not clear. Clear instructions for the safe/unsafe condition of release gear and hooks not posted inside the lifeboat. Lifeboat remote lowering wire bulldog gripes are wasted. Liferaft instructions not posted below Emergency light. Lifeboat davit remote lowering wire bulldog gripes are wasted     ","Miscellaneous","General Appearance","External Factors","","","","","instruction renewed, board oars marked, Lifeboat glass cleaned. instruction posted in lifeboat, bulldog grips renewed. Instruction posted under emgcy light. ","2024-09-10T23:59:35","","Completed","2024-08-20T23:59:35","No","No","No","Internal"]
[null,null,null,37013,11953,"106_Mon Aug 19 2024 19:07:29 GMT+0800","2024-08-10T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Midship locker – Alarm light indicators - name boards are rusted and faded.     ","Elect. Mach. & Equip.","General Appearance","External Factors","","","","","Painted and stenciled","2024-08-31T23:59:35","","Completed","2024-08-31T23:59:35","No","No","No","Internal"]
[null,null,null,37014,32855,"106_Mon Aug 19 2024 18:59:08 GMT+0800","2024-08-10T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Almost all Fire and foam hydrants on the deck were leaking.","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","Maintenance of the leaking hydrants carried out. No hydrants leaking now","2024-09-08T23:59:35","","Completed","2024-09-06T23:59:35","No","No","No","Internal"]
[null,null,null,37015,42130,"106_Mon Aug 19 2024 19:07:22 GMT+0800","2024-08-10T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Only a foam-type fire extinguisher was available in the forward store. DCP or CO2 fire extinguisher as per a recent circular was not available","Miscellaneous","General Appearance","Equipment Related","","","","","Appropriate extinguisher is already received at Singapore. Support bracket  fabricated and fitted.","2024-10-10T23:59:35","","Completed","2024-09-02T23:59:35","No","No","No","Internal"]
[null,null,null,37016,15111,"106_Mon Aug 19 2024 18:55:45 GMT+0800","2024-08-10T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Stbd Anchor was making a screeching sound when operated. To be investigated. A few Mooring winch brake bands in the forward area need de-rusting and painting.","Deck - Machinery","Mooring","Equipment Related","","","","","The screeching sound was investigated. Greasing of windlass was carried out. Old grease was removed completely and new grease was applied. The windlass was tested and found working satisfactorily. Brake band was de-rusted and painted","2024-08-31T23:59:35","","Completed","2024-08-31T23:59:35","No","No","No","Internal"]
[null,null,null,37017,10806,"0_Mon Aug 19 2024 19:21:17 GMT+0800","2024-08-10T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Many IMO symbols on deck are faded. IMO symbol for \"Number 6\" is not as per requirements.     ","LSA / FFA","General Appearance","Industry Issue","","","","","Faded IMO symbol on deck replaced, Number 6 colour photograph printed, laminated and posted","2024-08-31T23:59:35","","Completed","2024-08-31T23:59:35","No","No","No","Internal"]
[null,null,null,37425,35944,"106_Mon Sep 16 2024 01:17:57 GMT+0800","2024-09-09T23:59:35","Defect","Ship Staff","Ship Staff Insp.","FWG Distillate pump motor tripped on overload","","Eng. / Strg. Comp.","Equipment Related","10.31","Very High","","","Pump opened up and found impeller eroded and could have caused imbalance and vibration.Motor bearing end covers also worndown. Newly received motor is of different base and mounting has to be modified. Impoeller was replaced and for the time being we are running the FWG. New motor was received at Singapore and now the defect can be closed.","2024-12-21T23:59:35","PHAL240145 and PHAL245093","Completed","2024-12-03T23:59:35","No","No","No","Internal"]
[null,null,null,37421,27857,"106_Sun Sep 15 2024 19:02:51 GMT+0800","2024-09-10T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Aux Boiler Pilot burner Gas oil flexible line found damaged and leaking","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.31","Very High","","","Spare hose was requested and received at Le Havre. Defective hose was replaced and leakage rectified.","2024-10-16T23:59:35","PHAL240146","Completed","2024-09-29T23:59:35","No","No","No","Internal"]
[null,null,null,38002,48709,"106_Sat Oct 12 2024 19:28:05 GMT+0800","2024-09-28T23:59:35","Observation","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","DMITRY PETROV - 5.4.1 - Human // Senior Deck Officer: Not as expected.\nBull-dog clips fitted to the aft falls of the port side lifeboat were observed connected in a wrong way.","LSA / FFA","Safety / LSA / FFA","Human Error","5.1","Very High","","","Immediate Cause :\nFailure of the ship's safety inspection process to identify the incorrect connection of the bulldog clips on the aft falls of the port side lifeboat. Both the ship crew and safety officer did not detect this error during routine inspections.\nRoot Cause :\n1. Custom and practice surrounding use of procedures .\n2. Inadequate attention and thoroughness during safety inspections, leading to oversight. This human error resulted from complacency, rushed inspections, or a lack of focus on critical safety components, such as wire rope clips. Additionally, there has been inconsistent adherence to safety protocols or a lack of effective supervision during inspections, which allowed this issue to go unnoticed.","2024-10-26T23:59:35","","Completed","2024-10-11T23:59:35","No","No","No","External","Corrective Action\n1. Training has been provided to all crew members, including senior officers, on the proper safety inspection process to ensure that safety concerns are identified and addressed effectively.\n2. The safety inspection checklist has been updated to include specific checks for the correct installation of wire clips, including the correct number of clips and the required spacing between them.\n3. Posters and loss prevention materials have been displayed in common areas to assist the ship's crew in performing thorough and accurate safety inspections.\nPreventative Action :\n1. A detailed review of the ship safety inspection process will be carried out and all shortcomings will be addressed.\n2. Regular refresher training will be conducted onboard to ensure the Ship Safety inspections are carried out as required by the company procedures even after crew changes.\n3. Scenario-based training will be carried out where crew members are trained on spotting potential human errors in safety inspections, helping them become more aware of typical oversights and reinforcing the importance of vigilance.\n4. Crew members will be rotated during the inspections to prevent complacency from setting in due to familiarity with the tasks, ensuring fresh eyes and a renewed focus on each inspection.\n5. The findings will be shared among the fleet vessels to prevent recurrence"]
[null,null,null,38003,67958,"106_Sat Oct 12 2024 19:17:25 GMT+0800","2024-09-28T23:59:35","Observation","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","DMITRY PETROV - 5.4.1 - Lifeboats & Equipment: Maintenance task available – not completed. \nThree bull-dog clips connected to the aft falls of the port side lifeboat were observed connected to wire in a wrong way. U-bolts of wire rope clips were observed on the live end of the rope.","LSA / FFA","Safety / LSA / FFA","Equipment Related","5.1","Very High","","","Immediate Cause :\nThe U-bolts were wrongly positioned on the live end of the wire rope, deviating from standard procedure, likely due to a lack of attention or misinterpretation of the proper installation technique.\nRoot Cause :\nWe have completed the investigation into the incorrect installation of wire rope clips on the lifeboat davit and wish to inform you that, in June 2024, the wire clips were removed for maintenance on the wire and clips. However, after the maintenance work was completed, the clips were incorrectly reinstalled. This issue arose due to complacency, distractions, environmental factors, and a lack of proper supervision, which together contributed to a momentary oversight, resulting in the improper installation of wire clips.","2024-10-13T23:59:35","","Completed","2024-10-11T23:59:35","No","No","No","External","Corrective Action : \n1. The bulldog clips on the aft falls of the lifeboat were immediately reinstalled correctly, with the U-bolt positioned on the dead end and the saddle on the live end.\n2. The lifeboat wire was closely inspected for any damage caused by the improper installation of the wire rope clips. No damages were noted in the wire.\n3. On completion of the correct reinstallation of the wire rope clips, lifeboat lowering was carried out to verify the proper function of the falls and the overall safety of the lifeboat wire and davit.\nPreventative Action:\n1. The wire rope clips at all other locations onboard were verified for correct installation and were noted to be installed properly.\n2. Training was conducted for all officers on the correct rigging of wire rope clips as per company procedures. This also included information on the reduction in the load-bearing capacity of the wire rope due to improper installation of the clips and the required spacing between the wire clips and the number of wire clips necessary for the given wire size.\n3. Posters from COSWP Annex 18.2 – Bulldog Grips and loss prevention material from the P&I Club were posted in common areas to raise crew awareness on the correct rigging of wire rope clips.\n4. The findings will be shared among the fleet vessels to prevent recurrence"]
[null,null,null,38004,77430,"106_Sat Oct 12 2024 19:09:51 GMT+0800","2024-09-28T23:59:35","Observation","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","DMITRY PETROV - 2.8.1 - 1A.1.4 - Procedures and instructions are accessible: Procedure completeness/validity/version . The HVPQ published to the OCIMF website on 23-Sep-2024 was randomly reviewed the same day. Some questions were not responded, some questions were wrongly responded. For example: 1.2.4, 1.3.2, 1.4.2, 1.5.2, 1.5.4, 2.2.1, 4.1.1, 5.3.2, 8.3.8, 9.7.3,\n9.10.9, 9.15.4, 9.16.22, 10.1.3, 10.1.4, 10.1.7, 10.2.5, 11.3.1, 11.5.1, 13.1.4.","Documentation","Cert. & Docu.","Human Error","2.1","Very High","","","Immediate Cause:\nThe incorrect and blank responses in the HVPQ were due to a combination of officer oversight and a lack of clarity in understanding the questions, along with insufficient verification before PIQ submission.\nRoot Cause:\nWe have thoroughly investigated the observation and would like to inform you that, as correctly pointed out by the inspector, several responses in the HVPQ submission were either incorrect or left unanswered. Upon review, we found that some questions were left blank because they were not applicable to the vessel, while others were answered incorrectly due to an oversight by the\nofficers responsible for completing the HVPQ data and a misinterpretation of the questions. Additionally, we identified a lack of sufficient verification during the PIQ declaration, review, and operator declaration process. It was also noted that the OCIMF HVPQ6 desktop editor used was an outdated version.","2024-10-11T23:59:35","","Completed","2024-10-11T23:59:35","No","No","No","External","Corrective Action:\n1. The incorrect entries in the HVPQ have been corrected. Questions that were previously unanswered have now been marked as \"Not applicable.\"\n2. Training has been provided to the officers responsible for the HVPQ data input process, and they have been briefed on the correct interpretation of the questions. Additionally, they have been instructed to ensure that all fields are completed accurately and that non-applicable questions are properly addressed.\n3. Training has also been provided to implement a more robust verification process, which now includes a second-level review by a senior officer or designated verifier before submitting the PIQ declaration.\n4. The OCIMF HVPQ desktop software has been upgraded to Version V5.0.5.\n\nPreventive Action:\n1. Regular refresher training will be conducted onboard to ensure the accuracy of HVPQ data is maintained, even after crew changes.\n2. Officers have been briefed to refer to the company's documented procedures while completing the HVPQ information.\n3. The findings will be shared across all fleet vessels to prevent the recurrence of the observation and ensure that accurate HVPQ data is available to all parties.\n4. Checks will be conducted on the OCIMF HVPQ6 desktop software version across all fleet vessels, and it will be updated to the latest version. A robust process has been established to regularly verify the software version and implement updates as soon as a new version is released."]
[null,null,null,37997,49240,"106_Sun Nov 03 2024 20:54:34 GMT+0800","2024-10-28T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Bath area tiles of few cabins are loose and almost all cabins have mould deposit on the tiles.","Accommodation","General Appearance","Equipment Related","11.13","Low","","","Store for repairing and cleaning tiles have been requested and received at Singapore. The repair job were carried out and defects were rectified.","2025-03-01T23:59:35","PHAL240185","Completed","2025-01-03T23:59:35","No","No","No","Internal"]
[null,null,null,37998,56155,"106_Sun Nov 03 2024 20:44:17 GMT+0800","2024-10-28T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Water Boilers in both Pantries are not operational","Accommodation","General Appearance","Equipment Related","11.13","Low","","","Water tap of both water boilers were found damaged and spare valves were requested and received. Flushed the boiler with fresh water few times and then fitted the new valves and put the boilers in use.","2025-03-01T23:59:35","PHAL210190","Completed","2025-01-06T23:59:35","No","No","No","Internal"]
[null,null,null,37999,92335,"106_Sun Nov 03 2024 20:28:20 GMT+0800","2024-10-28T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Shower mixers of some cabins are leaking","Accommodation","General Appearance","Equipment Related","11.13","Low","","","What ever spare mixers vessel is having has been used to replace faulty mixers and spares for repairing remaining mixers has been raised. Received at Singapore and renewed.","2025-03-01T23:59:35","PHAL240185","Completed","2024-12-07T23:59:35","No","No","No","Internal"]
[null,null,null,38001,34286,"106_Fri Nov 15 2024 11:18:26 GMT+0800","2024-11-05T23:59:35","Defect","Ship Staff","Ship Staff Insp.","BWTS AFU was observed to be having SW leakage from tell tale hole at the foot of motor gear housing.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.8","Medium","","","Leakage from tell tale hole, indicates that the sealing ring on the drive shaft is leaking. It was tried by ship staff to take out the drive shaft, but the claw was found seized on the drive shaft. On consultation with maker, it was decided to wait for spares and once received the claw has to be broken to take out the shaft. Requisition raised for the recommended spares and were received at Singapore. The AFU was opened, the claw was cut off and removed. the claw shaft end was grinded to required dia and the gear box was removed and brought to E/R workshop. The sleeve was heated and removed from the driving shaft. With new spares the claw assembly was fitted back and after fitting the cover, FW was filled and checked for leaks and found none. Afterwards the gear box and motor were assembled and gear oil taken to required level. Shall observe the performance during next operation.","2025-03-01T23:59:35","PHAL240206","Completed","2025-01-04T23:59:35","No","No","No","Internal"]
[null,null,null,38000,63432,"106_Fri Nov 15 2024 10:48:19 GMT+0800","2024-11-09T23:59:35","Defect","Ship Staff","Ship Staff Insp.","VOCON System is not operational","Inert Gas","Cargo / Ballast Systems","Equipment Related","8.21","High","","","On inspection, the electric motor was found frozen. Same was removed and overhauled. The gears were found in good condition. After fitting the system back, operation was tested. Found that the pressure is holding when closed and opening confirmed by reducing the pressure setting. System is operational and the defect can be closed.","2025-03-01T23:59:35","","Completed","2024-11-29T23:59:35","No","No","No","Internal"]
[null,null,null,37996,58262,"106_Fri Nov 15 2024 11:07:23 GMT+0800","2024-11-12T23:59:35","Defect","Ship Staff","Ship Staff Insp.","BWTS Sludge pump coupling in Pump room is broken","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.8","Medium","","","New coupling was ordered and received . The pump, motor and intermediate coupling were removed, dissembled and shafts were checked for trueness. All found true. After overhauling except for the coupling all were fitted back. The pump shaft and intermediate shaft were found misaligned. The foundation is suspected to be deformed due to excessive tightening of discharge pipe flange. While dismantling the bunk head seal carbon ring was found broken, same was ordered and received and renewed.  The foundation raised part was removed and thinner plate was fitted. The pump was aligned  properly by inserting shims.  Foundation was tightened after aligning and then with new gaskets the flanges were tightened. Water was taken and checked for leaks and all were found normal. During next operation shall observe the performance.","2025-03-01T23:59:35","PHAL240137,  PHAL240212 and PHAL240195","Completed","2025-01-03T23:59:35","No","No","No","Internal"]
[null,null,null,39036,24695,"106_Thu Feb 13 2025 00:49:17 GMT+0800","2024-12-02T23:59:35","Defect","Ship Staff","Ship Staff Insp.","LT cooling expansion tank show sheen of Lub oil on top of water  surface.","Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.20","High","","","All AE LO cooler O-Rings renewed. Oil removed from system gradually.","2025-04-02T23:59:35","","Completed","2025-02-20T23:59:35","No","No","No","Internal"]
[null,null,null,38374,28058,"0_Sat Dec 14 2024 18:21:33 GMT+0800","2024-12-02T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Emergency DG room - co2 bottles cabinet door latch is damaged, and door is not closing properly.","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","Door repaired","2025-02-16T23:59:35","","Completed","2025-02-22T23:59:35","No","No","No","Internal"]
[null,null,null,38376,32407,"0_Sat Dec 14 2024 18:12:13 GMT+0800","2024-12-02T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Platform near funnel deck port side is having soot deposits and oily surface.","Miscellaneous","General Appearance","Behaviour Based","","","","","Funnel deck area thoroughly cleaned. All oily spots removed.","2024-12-12T23:59:35","","Completed","2024-12-12T23:59:35","No","No","No","Internal"]
[null,null,null,38377,61381,"0_Sat Dec 14 2024 15:21:52 GMT+0800","2024-12-02T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Nuts for holding the MOB light stbd side on bridge wing are corroded, bolts/nuts to be replaced with SUS.","LSA / FFA","Safety / LSA / FFA","Equipment Related","","","","","Bolts and nuts for MOB light stbd side on bridge wing replaced with SS Nuts & Bolts.","2024-12-09T23:59:35","","Completed","2024-12-08T23:59:35","No","No","No","Internal"]
[null,null,null,38378,70359,"0_Sat Dec 14 2024 18:24:44 GMT+0800","2024-12-02T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Most of the fair lead rollers on focsle deck are not rotating.","Deck - Mooring Machinery","General Appearance","Equipment Related","","","","","All fairlead rollers Fwd and Aft greased and rotated freely.","2024-12-17T23:59:35","","Completed","2024-12-14T23:59:35","No","No","No","Internal"]
[null,null,null,38379,79001,"0_Sat Dec 14 2024 18:19:23 GMT+0800","2024-12-02T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Engine room sky light door gasket is leaking.","Deck - Pipe / Fittings","ISM Related","Human Error","","","","","Wasted portion of the skylight gasket was cut and removed, new gasket with interlocking with old gasket fitted and rubber glue was used to join. After fitting no leaks observed.","2025-01-01T23:59:35","","Completed","2024-12-19T23:59:35","No","No","No","Internal"]
[null,null,null,38380,35995,"0_Sat Dec 14 2024 18:23:22 GMT+0800","2024-12-02T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Light above EMDG co2 room is filled with water.","Elect. Mach. & Equip.","ISM Related","Equipment Related","","","","","Light above emergency generator CO2 room cleaned and dried.","2024-12-09T23:59:35","","Completed","2024-12-08T23:59:35","No","No","No","Internal"]
[null,null,null,38381,98387,"106_Sat Dec 14 2024 15:20:35 GMT+0800","2024-12-02T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","One Pendant light on monkey island for the name board stbd side is having moisture","Elect. Mach. & Equip.","ISM Related","Equipment Related","","","","","The light fitting was opened , the glass globe was cleaned and silicon applied on the rubber gasket before fitting back.","2024-12-09T23:59:35","","Completed","2024-12-07T23:59:35","No","No","No","Internal"]
[null,null,null,38382,45237,"0_Sat Dec 14 2024 18:25:42 GMT+0800","2024-12-02T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Fwd hyd oil tank level gauge push button is seized and unable to press.","Deck - Mooring Machinery","ISM Related","Equipment Related","","","","","Hydraulic storage tank level gauge push button was freed and now can be pressed easily.","2024-12-17T23:59:35","","Completed","2024-12-07T23:59:35","No","No","No","Internal"]
[null,null,null,38383,13191,"106_Sat Dec 14 2024 18:16:26 GMT+0800","2024-12-02T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Galley cooking oven – bottom side is not working as reported by chief cook","Accommodation","MLC Related","Equipment Related","","","","","New heating element was received t Singapore and same was renewed. Cooking oven has been made operational","2025-01-16T23:59:35","","Completed","2024-12-11T23:59:35","No","No","No","Internal"]
[null,null,null,38384,48359,"0_Sat Dec 14 2024 18:17:20 GMT+0800","2024-12-02T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Galley exhaust manifold mesh is damaged at various locations","Accommodation","MLC Related","Equipment Related","","","","","New Mesh Installed.","2024-12-31T23:59:35","","Completed","2024-12-28T23:59:35","No","No","No","Internal"]
[null,null,null,38385,91908,"0_Sat Dec 14 2024 18:18:21 GMT+0800","2024-12-02T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Most of the gym equipment’s are not secured.","Accommodation","ISM Related","Behaviour Based","","","","","All Gym equipment's well secured.","2024-12-16T23:59:35","","Completed","2024-12-15T23:59:35","No","No","No","Internal"]
[null,null,null,38386,51813,"106_Mon Jan 06 2025 19:50:12 GMT+0800","2024-12-02T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","FO sludge tank level gauge is not working.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.31","Very High","","","The gauge wire connecting to bob was slipped from the pulley and not moving. Same was fitted correctly and now the gauge is operational.","2025-01-01T23:59:35","","Completed","2024-12-11T23:59:35","No","No","No","Internal"]
[null,null,null,38387,30294,"106_Mon Jan 06 2025 19:17:01 GMT+0800","2024-12-02T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Aux. Engine No.3 LO cooler is leaking in to LT side.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.31","Very High","","","At anchorage, the cooler o-rings were renewed and oil from system skimmed off. After that chemical was added in to system and drained from equipment ion the system.","2025-01-01T23:59:35","","Completed","2024-12-28T23:59:35","No","No","No","Internal"]
[null,null,null,38388,14386,"106_Mon Jan 06 2025 19:37:24 GMT+0800","2024-12-02T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Donkey boiler local control panel to be covered with plate for protecting against water spray.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.31","Very High","","","Metal sheet was introduced on top of the panel, so that water spray from SW pipe will not fall on the panel.","2025-01-16T23:59:35","","Completed","2025-01-04T23:59:35","No","No","No","Internal"]
[null,null,null,38389,37932,"106_Mon Jan 06 2025 19:44:57 GMT+0800","2024-12-02T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Lub oil leak form ME lub oil backwash filter.","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.31","Very High","","","At Khor Al Subair, the LO backwash filter was cleaned and at the same time, the leakage was rectified by renewing the top o-ring.","2025-01-16T23:59:35","","Completed","2024-12-24T23:59:35","No","No","No","Internal"]
[null,null,null,39295,28519,"106_Fri Mar 07 2025 23:05:27 GMT+0800","2024-12-16T23:59:35","Defect","Ship Staff","Ship Staff Insp.","EGCS SW feed PP#1 VFD unit defective","E/R - Main Engine","MARPOL Related","Equipment Related","10.20","High","","","Presently SW pump is operated in VFD bypass mode. Communication withe office is in progress. Spares received this call Singapore communication with maker in progress for installation of the same. Troubleshooting carried out and presently VFD working fine","2025-06-01T23:59:35","","Completed","2025-06-09T23:59:35","No","No","No","Internal","VFD being sourced & will be connected at next convenient port."]
[null,null,null,39040,86816,"106_Thu Feb 13 2025 00:52:35 GMT+0800","2025-01-02T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Fwd Hyd Oil System Oil sample showing Caution for water content","Deck - Machinery","Mooring","Equipment Related","","","","","Vent valve replaced. Oil treated in storage tank. Presently by onboard test the water content has reduced to less than 0.02%. LO sample has been landed for shore analysis. Shall close out the job once shore results has come. LO test result indicated water content negligible","2025-04-02T23:59:35","","Completed","2025-04-10T23:59:35","No","No","No","Internal","Pls confirm issue has been sorted out, accordingly update the job."]
[null,null,null,38375,23998,"106_Sun Jan 05 2025 18:09:10 GMT+0800","2025-01-03T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Forward fire wire motor air filter found broken and need to be replaced.","Deck - Mooring Machinery","Mooring","Equipment Related","","","","","Vessel received new air filter for forward fire wire at Singapore on 30 Jan 2025.\nSame has been replaced with new filter. Operation checked. All in good order.","2025-03-31T23:59:35","PHAL250008","Completed","2025-02-05T23:59:35","No","No","No","Internal"]
[null,null,null,39046,61661,"106_Thu Feb 13 2025 01:29:54 GMT+0800","2025-01-09T23:59:35","Defect","Ship Staff","Ship Staff Insp.","No.1 Ballast pump discharge pipe section is leaking","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","Permanent repairs carried out","2025-05-02T23:59:35","","Completed","2025-02-10T23:59:35","No","No","No","Internal"]
[null,null,null,39037,72697,"106_Tue Feb 11 2025 17:19:11 GMT+0800","2025-01-31T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Port side HHC light and hooter base plate broken and needs to repair the same.\nAll HHC and provision crane Light and hooter to check for proper functioning.","Deck - Machinery","ISM Related","Equipment Related","","","","","HOOTER BASE  REPAIRED.","2025-04-16T23:59:35","","Completed","2025-04-11T23:59:35","No","No","No","Internal","Its long pending observation, pls let us know vsl plan to repair it."]
[null,null,null,39048,38989,"106_Thu Feb 13 2025 00:57:13 GMT+0800","2025-02-22T23:59:35","Defect","Ship Staff","Ship Staff Insp.","AE # 2 fuel oil inlet temperature sensor found defective.","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.3","Medium","","","Fuel oil inlet temperature sensor received and same renewed, working satisfactory","2025-05-30T23:59:35","PHAL240172","Completed","2025-05-30T23:59:35","No","No","No","Internal","Spare will be connected at Singapore on 07Th May"]
[null,null,null,39045,87776,"106_Thu Feb 13 2025 00:15:08 GMT+0800","2025-02-23T23:59:35","Defect","Ship Staff","Ship Staff Insp.","EGCS A/E Scrubber exhaust outlet funnel spark arrester is damaged.","Miscellaneous","General Appearance","Equipment Related","10.20","High","","","EGCS A/E Scrubber exhaust outlet funnel spark arrester mesh fabricated.","2025-05-22T23:59:35","","Completed","2025-05-16T23:59:35","No","No","No","Internal","Vsl to carryout job at next opportunity during anchorage in Brazil."]
[null,null,null,37424,49335,"106_Sun Sep 15 2024 18:33:10 GMT+0800","2025-02-27T23:59:35","Defect","Ship Staff","Ship Staff Insp.","Sewage plant chemical dosing pump is defective","E/R - Pumps,Miscellaneous","Eng. / Strg. Comp.","Equipment Related","10.31","Very High","","","COMPLETE CHEMICAL DOSING PUMP REPLACED WITH SPARE NEW ONE RECEIVED IN SINGAPORE .","2025-05-26T23:59:35","PHAL240147","Completed","2025-05-12T23:59:35","No","No","No","Internal","Spare will be connected at Singapore on 07Th May"]
[null,null,null,39296,84290,"106_Fri Mar 07 2025 23:02:22 GMT+0800","2025-03-04T23:59:35","Defect","Ship Staff","Ship Staff Insp.","IG platform O2 sensor defective","Inert Gas","Eng. / Strg. Comp.","Equipment Related","10.20","High","","","SENSER RENEWED WITH SAPRE NEW ONE RECEIVED IN SINGAPORE","2025-06-01T23:59:35","","Completed","2025-05-20T23:59:35","No","No","No","Internal","Sensor ready in Singapore & will be connected on 07th May"]
[null,null,null,39044,75397,"106_Thu Feb 13 2025 01:28:41 GMT+0800","2025-03-06T23:59:35","Defect","Ship Staff","Ship Staff Insp.","IG valve indicators are an Ex-rated explosion-proof type. Many screws are missing. IG valve indicators plastic cover showing brittle marks","Deck - Pipe / Fittings","General Appearance","Equipment Related","","","","","Spares received. Renewal of VV position indicator covers .","2025-06-04T23:59:35","PHAL240193","Completed","2025-05-20T23:59:35","No","No","No","Internal","Spare will be connected at Singapore on 07Th May"]
[null,null,null,37018,92920,"0_Mon Aug 19 2024 19:11:34 GMT+0800","2025-03-10T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","IG valve indicators are an Ex-rated explosion-proof type. Many screws are missing. IG valve indicators plastic cover showing brittle marks","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","8.25","Very High","","","IG valves to be inspected. Spares to be ordered and valves repaired once the spares are received. Need the diagram and parts catalogue for ordering the spares.\nReceived spares in Singapore same replaced. Presently all indicators are fine","2025-06-08T23:59:35","PHAL240193- Cancelled\nPHAL250169 - Confirmed","Completed","2025-05-15T23:59:35","No","No","No","Internal","Spare will be connected at Singapore on 07Th May"]
[null,null,null,40191,68409,"106_Tue Apr 08 2025 00:49:11 GMT+0800","2025-03-24T23:59:35","Critical Equipment","Ship Staff","Ship Staff Insp.","GMDSS Battery charger unit defective. Due to burnt Battery charger NBB-724 at anchorage.","Navigation - GMDSS & Communication","Navigation","Equipment Related","4.23","High","","","To replace NBB-724 battery charger unit awaiting spares. \nSpares could not be connected at MADRE DE DEUS will be connected at next port.\nEECEIVED SPARE AT SINGAPORE MAY 2025 SAME REPLACED SYSTEM WORKING FINE","2025-05-26T23:59:35","","Completed","2025-05-08T23:59:35","No","No","No","Internal","Spares connected at Singapore on 07th May, pls close job after installing new parts."]
[null,null,null,40322,48265,"106_Sat Apr 19 2025 22:41:15 GMT+0800","2025-04-11T23:59:35","Defect","Ship Staff","Ship Staff Insp.","VECS O2 sensor showing faulty reading.","Miscellaneous","Cargo / Ballast Systems","Equipment Related","8.42","Medium","","","SENSOR RENEWD ","2025-06-11T23:59:35","PHAL250016","Completed","2025-05-24T23:59:35","No","No","No","Internal","Spares will be connected this call Singapore - 07th May"]
[null,null,null,40598,29812,"106_Wed May 14 2025 17:55:58 GMT+0800","2025-05-08T23:59:35","Observation","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","There were no records available to confirm that the accuracy of the echo sounder had been confirmed by periodic comparison in\naccordance with company procedures which has to be completed every 6 months.\nBy Capt. Paveen Bajaj.","Navigation - Echo Sounder / Speed Log","Cert. & Docu.","Human Error","4.1","High","","","Last test of echo sounder accuracy was taken on 21st. Oct. 2024. Due to long voyage of the vessel from 3rd. Apr 2025 to 6th. May 205 this could not be carried out.\n\nImmediate Cause: Company Standard, policy or administrative control not used. \n\nRoot Cause: Last test of echo sounder accuracy was taken on 21st. Oct. 2024. Due to long voyage of the vessel from 3rd. Apr 2025 to 6th. May 205 this could not be carried out.  \n\nImmediately deck officer were asked to carried out sounding of vessel with hand lead line and check for accuracy of echo sounder. At JPUT Berth J2.","2025-05-28T23:59:35","","Completed","2025-05-08T23:59:35","No","No","No","External","Corrective Action: Immediately deck officer were asked to carried out sounding of vessel with hand lead line and check for accuracy of echo sounder. At JPUT Berth J2\n\nPreventive action: Company procedure explained to all deck officers. The Echosounder’s accuracy shall be verified when compared to water of a known depth using a hand lead line, when possible, but at least once every 6 months. (Procedure:  12.01.04.08.00 – ECHO SOUNDER).  "]
[null,null,null,40599,50454,"106_Wed May 14 2025 17:59:25 GMT+0800","2025-05-08T23:59:35","Observation","SIRE / CDI Insp.","OM Insp. (Eg. SIRE / CDI etc.)","Familiarization record of visiting marine superintendent (07 Aug 2024 to 09 Aug 2024) was not available as required by company procedure. \nBy Capt. Paveen Bajaj.","Documentation","Cert. & Docu.","Human Error","3.5","Medium","","","The deck team should be familiar with the company procedures wrt familiarization of all shipboard as well as visitors and  contractors\n\nImmediate Cause: Company Standard, policy or administrative control not used. \n\nRoot Cause: Unaware of SPACs\n\nDiscussed with all senior and junior officers on board and training given so that familiarization of visitors and contractors is not missed. All records to be properly maintained","2025-05-28T23:59:35","","Completed","2025-05-10T23:59:35","No","No","No","External","Corrective Action: The deck team should be familiar with the company procedures wrt familiarisation of all shipboard as well as visitors and  contractors. \n\nPreventive action: Discussed with all senior and junior officers on board and training given so that familiarisation of visitors and contractors is not missed. All records to be properly maintained. \n"]
[null,null,null,40607,15142,"106_Thu Jun 05 2025 23:23:29 GMT+0800","2025-05-17T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Stbd. Side Pilot ladder motor cover wasted. To renew. ","Deck - Machinery","General Appearance","Equipment Related","5.47","Medium","","","Stbd. Side Pilot ladder motor cover wasted. To renew. //\nNew  motor cover fabricated and installed in place.","2025-06-17T23:59:35","","Completed","2025-05-28T23:59:35","No","No","No","Internal"]
[null,null,null,40608,88424,"106_Thu Jun 05 2025 23:26:30 GMT+0800","2025-05-17T23:59:35","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Manifold drip tray Gratings port and stbd. Require maintenance. ","Deck - Pipe / Fittings","General Appearance","External Factors","6.6","Medium","","","Manifold drip tray Gratings port and stbd removed from place derusted and new paint coat applied. Some bent portions straightened up","2025-06-17T23:59:35","","Completed","2025-05-26T23:59:35","No","No","No","Internal"]
[null,null,null,40609,90718,"106_Thu Jun 05 2025 23:30:40 GMT+0800","2025-05-17T23:59:35","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","China passage requires derusting and painting. ","Miscellaneous","General Appearance","External Factors","11.3","Medium","","","China passage are maintenance carried out and same painted. Presently in good appealing condition.","2025-06-17T23:59:35","","Completed","2025-05-21T23:59:35","No","No","No","Internal"]
[null,null,null,40610,41632,"106_Thu Jun 05 2025 23:28:27 GMT+0800","2025-05-17T23:59:35","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Fore peak store Bulkhead has lots of dust settled require extensive cleaning. ","Miscellaneous","General Appearance","External Factors","11.12","Low","","","Fore peak store Bulkhead cleaned mopped and presently in good condition","2025-06-01T23:59:35","","Completed","2025-05-20T23:59:35","No","No","No","Internal"]
[null,null,null,40611,99122,"106_Thu Jun 05 2025 23:32:19 GMT+0800","2025-05-17T23:59:35","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Garbage locker require derusting and painting. ","Miscellaneous","General Appearance","External Factors","6.2","High","","","Garbage locker arranged properly cleaned and painted . Presently in good condition.","2025-06-17T23:59:35","","Completed","2025-05-27T23:59:35","No","No","No","Internal"]
[null,null,null,40612,58747,"106_Thu Jun 05 2025 23:34:00 GMT+0800","2025-05-17T23:59:35","Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Poster to be placed on Windlass “To operate Windlass in Low speed”.","Deck - Machinery,Deck - Mooring Machinery","Mooring","Equipment Related","9.24","Medium","","","Poster placed on Windlass “To operate Windlass in Low speed”.","2025-05-27T23:59:35","","Completed","2025-05-19T23:59:35","No","No","No","Internal"]
[null,null,null,40613,78045,"106_Thu Jun 05 2025 23:36:48 GMT+0800","2025-05-17T23:59:35","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Dust accumulation in IG platform area to be cleared.","Miscellaneous","General Appearance","External Factors","10.29","Medium","","","Dust accumulation in IG platform  cleared and mopped. Presently in good condition..","2025-06-01T23:59:35","","Completed","2025-05-20T23:59:35","No","No","No","Internal"]
[null,null,null,40614,62620,"106_Thu Jun 05 2025 23:43:39 GMT+0800","2025-05-17T23:59:35","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Grinder machine bulb found fused in Engine room workshop need to replace.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","External Factors","10.37","Medium","","","Grinder machine bulb renewed with new bulb","2025-06-01T23:59:35","","Completed","2025-05-18T23:59:35","No","No","No","Internal"]
[null,null,null,40615,56787,"106_Thu Jun 05 2025 23:38:06 GMT+0800","2025-05-17T23:59:35","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Turning gear teeth needs greasing.","E/R - Main Engine","Eng. / Strg. Comp.","External Factors,Equipment Related","10.29","Medium","","","Turning gear teeth  greasing. carried out.","2025-06-01T23:59:35","","Completed","2025-05-21T23:59:35","No","No","No","Internal"]
[null,null,null,40616,39857,"106_Thu Jun 05 2025 23:35:20 GMT+0800","2025-05-17T23:59:35","Other","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Electrical panel in the boiler platform needs to be curtained with plastic.","Elect. Mach. & Equip.","Eng. / Strg. Comp.","External Factors","10.29","Medium","","","Electrical panel in the boiler platform  curtained with plastic.","2025-06-01T23:59:35","","Completed","2025-05-20T23:59:35","No","No","No","Internal"]
[null,null,null,40617,32167,"106_Thu Jun 05 2025 23:39:51 GMT+0800","2025-05-17T23:59:35","Defect,Observation","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Workshop welding curtain needs to be replaced as same short and having some holes.","Miscellaneous","Safety / LSA / FFA","External Factors","10.29","Medium","","","Workshop welding curtain renewed with new curtain","2025-06-01T23:59:35","","Completed","2025-05-19T23:59:35","No","No","No","Internal"]
[null,null,null,null,90757,"106_Thu Jun 05 2025 23:42:17 GMT+0800","2025-05-17T08:00:00","Defect","Owner / Marine / Tech. Suptd.","Suptd. Insp.","Bunker line filter inlet v/v actuator body damaged, same repaired. Requisition raised for the same.","Deck - Pipe / Fittings","MARPOL Related","External Factors","6.7","High","","","NEW ACTUATOR INSTALLED IN DD ","2025-07-17T08:00:00","","Completed",null,"No","No","No","Internal",""]
[null,null,null,null,74876,"106_Thu Feb 13 2025 01:05:07 GMT+0800","2025-03-16T08:00:00","Defect","Ship Staff","Ship Staff Insp.","ME HP SCR in-operational","E/R - Main Engine","MARPOL Related","Equipment Related","10.26","High","","","SCR TESTED AND MADE OPERATIONAL. ","2025-06-14T08:00:00","250215","Completed","2025-08-12T08:00:00","No","No","No","Internal",""]
[null,null,null,null,70047,"106_Thu Feb 13 2025 00:55:06 GMT+0800","2025-03-13T08:00:00","Defect","Ship Staff","Ship Staff Insp.","AE#1 TC inlet temperature sensor faulty","E/R - Aux. Engine","Eng. / Strg. Comp.","Equipment Related","10.2","Low","","","NEW SENSOR RECEIVED AND RENEWED. ","2025-06-11T08:00:00","PHAL250045","Completed","2025-08-06T08:00:00","No","No","No","Internal","Spare will be connected at next convenient port"]
[null,null,null,null,30308,"106_Thu Feb 13 2025 00:22:48 GMT+0800","2025-03-11T08:00:00","Defect","Ship Staff","Ship Staff Insp.",".AE Fuel circulating PP leaking from changeover valve while in LSMGO","E/R - Pipes/ valves & fittings,E/R - Pumps","Eng. / Strg. Comp.","Equipment Related","10.20","High","","","CHANGE OVER UNIT OVERHAULED WITH SPARES AND LEAKAGE STOPPED. ","2025-06-05T08:00:00","PHAL250039","Completed","2025-08-04T08:00:00","No","No","No","Internal","Spares sourced & will be connected at next convenient port."]
[null,null,null,null,17178,"106_Thu Feb 13 2025 01:27:01 GMT+0800","2025-01-06T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Cargo sea chest valve COV069 observed not holding, suspecting damaged seat ring.","Cargo Mach.","Cargo / Ballast Systems","Equipment Related","","","","","NEW SEA CHEST VALVE SEAT RENEWED IN DD ","2025-08-07T08:00:00","","Completed","2025-07-30T08:00:00","No","No","No","Internal","Job will be carried out in DD in June'25"]
[null,null,null,null,55002,"106_Thu Feb 13 2025 01:07:23 GMT+0800","2025-02-27T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Aux. Boiler # 1 Bellow found defective.","E/R - Boiler","Eng. / Strg. Comp.","Equipment Related","10.3","Medium","","","NEW BELLOW  INSTALLED ","2025-05-26T08:00:00","PHAL250021","Completed","2025-08-06T08:00:00","No","No","No","Internal","Spares will be connected at next convenient port."]
[null,null,null,null,23124,"106_Thu Feb 13 2025 00:41:40 GMT+0800","2025-02-28T08:00:00","Defect","Ship Staff","Ship Staff Insp.","ME LO backwash filter found leaking from changeover lever shaft","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.20","High","","","SPARES RECEIVED IN DD AND CHANGE VOER SHAFT OVERHAULED. ","2025-05-27T08:00:00","PHAL250032","Completed","2025-08-03T08:00:00","No","No","No","Internal","Spares will be connected to vsl at next convenient port."]
[null,null,null,null,66799,"106_Fri Mar 07 2025 22:59:50 GMT+0800","2025-03-03T08:00:00","Defect","Ship Staff","Ship Staff Insp.","EGCS sealing air fan#1 expansion bellow(Metal) found cracked","E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.2","Low","","","NEW BELLOW INSTALLED IN DD ","2025-06-01T08:00:00","PHAL250168","Completed","2025-07-27T08:00:00","No","No","No","Internal","Spare will be connected at next convenient port"]
[null,null,null,null,71468,"106_Fri Mar 07 2025 22:56:25 GMT+0800","2025-03-03T08:00:00","Defect","Ship Staff","Ship Staff Insp.","EGCS differential pressure transmitter PT 123 & PT123B 2 nos faulty","E/R - Main Engine","MARPOL Related","Equipment Related","10.2","Low","","","NEW SENSOR INSTALLED AND WORKING IN GOOD ORDER. ","2025-06-01T08:00:00","PHAL250178- EGCS GE SCRUBBER INSTRUMENTATION SPARES","Completed","2025-07-29T08:00:00","No","No","No","Internal","Spare will be connected at next convenient port."]
[null,null,null,null,94054,"106_Sun Nov 03 2024 20:09:12 GMT+0800","2025-03-02T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Fwd HPU No.1 is not developing pressure.","Deck - Mooring Machinery","Mooring","Equipment Related","9.14","Medium","","","NCS TECH. ATTENDED THE VESSEL IN DD AND RESOLVED ALL THE ISSUES. ","2025-05-31T08:00:00","PHAL240177/2","Completed","2025-07-29T08:00:00","No","No","No","Internal","Spares will be connected to vsl at next convenient port."]
[null,null,null,null,48782,"0_Tue Jul 16 2024 08:16:48 GMT+0800","2025-02-28T08:00:00","Defect","Ship Staff","Ship Staff Insp.","Main Engine Lub Oil Autoback wash filter change over cock is not holding and so Bypass filter unable to clean.","Deck - Pipe / Fittings,E/R - Pipes/ valves & fittings","Eng. / Strg. Comp.","Equipment Related","10.28","Low","","","O RING RENEWED AND LEAK RECTIFIED. ","2025-05-27T08:00:00","PHAL250032","Completed","2025-08-06T08:00:00","No","No","No","Internal","Spares will be connected to vsl at next convenient port."]

{"sheet":"Calc","index":2,"n_rows":28,"n_cols":12,"rows_kept":28,"cut":false,"hidden":true,"merged":[]}
["Def_type","Def_cause","Equipments","VIQrefno","Observer_code"]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,"Dim itemSele As Long"]
[null,null,null,null,null,null,null,null,null,null,null,"   dim startRow as integer"]
[null,null,null,null,null,null,null,null,null,null,null,"   startRow=1"]
[null,null,null,null,null,null,null,null,null,null,null,"        For itemSele = 0 To ListBox1.ListCount - 1"]
[null,null,null,null,null,null,null,null,null,null,null,"        If ListBox1.Selected(itemSele) = True Then"]
[null,null,null,null,null,null,null,null,null,null,null,"        Worksheets(\"WorksheetName\").Range(\"A\" & startRow).Value = ListBox1.List(itemSele)"]
[null,null,null,null,null,null,null,null,null,null,null,"        startRow = startRow + 1"]
[null,null,null,null,null,null,null,null,null,null,null,"        End If"]
[null,null,null,null,null,null,null,null,null,null,null,"        Next"]
[null,null,null,null,null,null,null,null,null,null,null,"Dim LastRowA As String"]
[null,null,null,null,null,null,null,null,null,null,null,"        Dim itemSele As Long"]
[null,null,null,null,null,null,null,null,null,null,null,"       Dim startRow as integer"]
[null,null,null,null,null,null,null,null,null,null,null,"        LastRowA = ActiveSheet.Cells(Rows.count, \"A\").End(xlUp).row"]
[null,null,null,null,null,null,null,null,null,null,null,"        startQue = 0"]
[null,null,null,null,null,null,null,null,null,null,null,"        For itemSele = 0 To ListBox1.ListCount - 1"]
[null,null,null,null,null,null,null,null,null,null,null,"        For startRow = 1 To LastRowA"]
[null,null,null,null,null,null,null,null,null,null,null,"        If Worksheets(\"WorksheetName\").Range(\"A\" & startRow).Value = ListBox1.List(itemSele) Then"]
[null,null,null,null,null,null,null,null,null,null,null,"        ListBox1.Selected(itemSele) = True"]
[null,null,null,null,null,null,null,null,null,null,null,"        Exit For"]
[null,null,null,null,null,null,null,null,null,null,null,"        End If"]
[null,null,null,null,null,null,null,null,null,null,null,"        Next j"]
[null,null,null,null,null,null,null,null,null,null,null,"        Next"]
[null,null,null,null,null,null,null,null,null,null,null,"        End If"]

{"sheet":"Areaofobs","index":3,"n_rows":17,"n_cols":2,"rows_kept":17,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Cargo / Ballast Systems",11]
["Cert. & Docu.",2]
["Communication",6]
["Crew Management",3]
["Emgcy. Systems",13]
["Eng. / Strg. Comp.",14]
["General Appearance",15]
["Ice Opns.",17]
["ISM Related",7]
["ISPS Related",10]
["MARPOL Related",9]
["MLC Related",4]
["Mooring",12]
["Navigation",5]
["Safety / LSA / FFA",8]
["Structural Condn. / WT integrity ",16]

{"sheet":"Vessel_type","index":4,"n_rows":1,"n_cols":2,"rows_kept":1,"cut":false,"hidden":true,"merged":[]}
["Vessel_type","ID"]

{"sheet":"Deficiency_type","index":5,"n_rows":8,"n_cols":3,"rows_kept":8,"cut":false,"hidden":true,"merged":[]}
["TITLE","Type of deficiency_description","ID"]
["Breakdown",null,6]
["Critical Equipment",null,4]
["Defect",null,1]
["Guarantee Claim",null,8]
["Non Conformity",null,2]
["Observation",null,3]
["Other",null,7]

{"sheet":"VIQrefno","index":6,"n_rows":427,"n_cols":3,"rows_kept":427,"cut":false,"hidden":true,"merged":[]}
["VIQ_ref_no","Risk Value of observation","ID"]
["1.1","Low",8243]
["1.10","Low",8252]
["1.11","Low",8253]
["1.12","Low",8254]
["1.13","Low",8255]
["1.14","Low",8256]
["1.15","Low",8257]
["1.16","Low",8259]
["1.17","Low",8260]
["1.18","Low",8261]
["1.19","Low",8262]
["1.2","Low",8244]
["1.20","Low",8263]
["1.21","Low",8265]
["1.22","Low",8266]
["1.23","Low",8267]
["1.24","Low",8268]
["1.25","Low",8269]
["1.26","Low",8270]
["1.3","Low",8245]
["1.4","Low",8246]
["1.5","Low",8247]
["1.6","Low",8248]
["1.7","Low",8249]
["1.8","Low",8250]
["1.9","Low",8251]
["1.99","High",11258]
["10.1","Medium",8461]
["10.10","High",8470]
["10.11","Medium",8471]
["10.12","Very High",8472]
["10.13","Very High",8473]
["10.14","Medium",8474]
["10.15","Low",8475]
["10.16","Very High",8476]
["10.17","Very High",8477]
["10.18","High",8478]
["10.19","Very High",8479]
["10.2","Low",8462]
["10.20","High",8480]
["10.21","Medium",8481]
["10.22","Low",8482]
["10.23","Medium",8483]
["10.24","Low",8484]
["10.25","Very High",8485]
["10.26","High",8486]
["10.27","Medium",8487]
["10.28","Low",8488]
["10.29","Medium",8489]
["10.3","Medium",8463]
["10.30","High",8490]
["10.31","Very High",8491]
["10.32","Very High",8492]
["10.33","High",8493]
["10.34","High",8494]
["10.35","Very High",8495]
["10.36","Very High",8496]
["10.37","Medium",8497]
["10.38","Medium",8498]
["10.39","High",8499]
["10.4","High",8464]
["10.40","Medium",8500]
["10.41","Medium",8501]
["10.42","Medium",8502]
["10.43","Medium",8503]
["10.44","Medium",8504]
["10.45","Very High",8505]
["10.46","High",8506]
["10.47","Medium",8507]
["10.48","High",8508]
["10.49","Medium",8509]
["10.5","Low",8465]
["10.50","High",8510]
["10.51","Low",8511]
["10.52","Medium",8512]
["10.53","Medium",8513]
["10.54","High",8514]
["10.55","Low",8515]
["10.6","Very High",8466]
["10.7","Medium",8467]
["10.8","Medium",8468]
["10.9","Medium",8469]
["10.99","High",8516]
["11.1","High",8420]
["11.10","Medium",8429]
["11.11","Very High",8430]
["11.12","Low",8431]
["11.13","Low",8432]
["11.14","Medium",8433]
["11.15","Low",8434]
["11.16","Low",8435]
["11.17","Low",8436]
["11.2","Medium",8421]
["11.3","Medium",8422]
["11.4","Very High",8423]
["11.5","Medium",8424]
["11.6","Medium",8425]
["11.7","High",8426]
["11.8","Low",8427]
["11.9","Low",8428]
["11.99","High",8437]
["12.1","High",8438]
["12.10","High",8448]
["12.11","High",8449]
["12.12","High",8450]
["12.13","High",8451]
["12.14","High",8452]
["12.15","High",8453]
["12.16","High",8454]
["12.17","High",8455]
["12.18","High",8456]
["12.19","High",8457]
["12.2","High",8439]
["12.20","High",8458]
["12.21","High",8459]
["12.3","High",8441]
["12.4","High",8442]
["12.5","High",8443]
["12.6","High",8444]
["12.7","High",8445]
["12.8","High",8446]
["12.9","High",8447]
["12.99","High",8460]
["2.1","Very High",8296]
["2.1.9","Very High",11259]
["2.10","Medium",8304]
["2.11","Medium",8305]
["2.12","Low",8306]
["2.13","Low",8307]
["2.14","Low",8308]
["2.15","Low",8309]
["2.16","Medium",8310]
["2.2","Medium",8297]
["2.3","High",8295]
["2.4","Medium",8298]
["2.5","Medium",8299]
["2.6","Low",8300]
["2.7","High",8301]
["2.8","High",8302]
["2.9","Medium",8303]
["2.99","High",8311]
["3.1","High",8312]
["3.2","Very High",8313]
["3.3","High",8314]
["3.4","Low",8294]
["3.5","Medium",8315]
["3.6","High",8316]
["3.7","Very High",8317]
["3.8","Very High",8318]
["3.99","High",8319]
["4.1","High",8320]
["4.10","High",8329]
["4.11","Medium",8330]
["4.12","Very High",8331]
["4.13","Very High",8332]
["4.14","Very High",8333]
["4.15","Very High",8334]
["4.16","Very High",8335]
["4.17","Very High",8336]
["4.18","Very High",8337]
["4.19","Low",8338]
["4.2","Medium",8321]
["4.20","Very High",8339]
["4.21","High",8340]
["4.22","Low",8341]
["4.23","High",8342]
["4.24","High",8343]
["4.25","Low",8344]
["4.26","Low",8345]
["4.27","High",8346]
["4.3","Medium",8322]
["4.4","High",8323]
["4.5","Very High",8324]
["4.6","Medium",8325]
["4.7","High",8326]
["4.8","Medium",8327]
["4.9","Medium",8328]
["4.99","High",8347]
["5.1","Very High",8517]
["5.10","High",8526]
["5.11","Low",8527]
["5.12","Medium",8528]
["5.13","High",8529]
["5.14","Very High",8530]
["5.15","Medium",8531]
["5.16","Very High",8532]
["5.17","Very High",8533]
["5.18","High",8534]
["5.19","Medium",8535]
["5.2","Very High",8518]
["5.20","Medium",8536]
["5.21","Medium",8537]
["5.22","High",8539]
["5.23","Very High",8540]
["5.24","Very High",8541]
["5.25","Medium",8542]
["5.26","Medium",8543]
["5.27","Medium",8544]
["5.28","Very High",8545]
["5.29","High",8546]
["5.3","Low",8519]
["5.30","High",8547]
["5.31","High",8548]
["5.32","High",8549]
["5.33","High",8550]
["5.34","Low",8551]
["5.35","Medium",8552]
["5.36","Low",8553]
["5.37","Low",8554]
["5.38","High",8555]
["5.39","Very High",8556]
["5.4","High",8520]
["5.40","Very High",8557]
["5.41","Very High",8558]
["5.42","Medium",8559]
["5.43","High",8560]
["5.44","High",8561]
["5.45","Medium",8564]
["5.46","Medium",8565]
["5.47","Medium",8566]
["5.48","Medium",8567]
["5.5","Low",8521]
["5.6","Low",8522]
["5.7","Medium",8523]
["5.8","Medium",8524]
["5.9","Very High",8525]
["5.99","High",8568]
["6.1","Medium",8348]
["6.10","Low",8357]
["6.11","High",8358]
["6.12","Medium",8359]
["6.13","Low",8360]
["6.14","High",8361]
["6.15","High",8362]
["6.16","Very High",8363]
["6.17","Very High",8364]
["6.18","Medium",8365]
["6.19","Low",8366]
["6.2","High",8349]
["6.20","Medium",8367]
["6.21","High",8368]
["6.22","Medium",8369]
["6.3","Low",8350]
["6.4","High",8351]
["6.5","Medium",8352]
["6.6","Medium",8353]
["6.7","High",8354]
["6.8","High",8355]
["6.9","Low",8356]
["6.99","High",8370]
["7.1","High",8371]
["7.10","High",8380]
["7.11","High",8381]
["7.12","High",8382]
["7.13","Medium",8383]
["7.14","Medium",8384]
["7.15","High",8385]
["7.16","High",8386]
["7.17","High",8387]
["7.2","High",8372]
["7.3","Low",8373]
["7.4","Low",8374]
["7.5","Low",8375]
["7.6","Medium",8376]
["7.7","Low",8377]
["7.8","High",8378]
["7.9","High",8379]
["7.99","High",8388]
["8.1","Very High",8569]
["8.10","Very High",8578]
["8.100","Low",11227]
["8.101","Medium",11228]
["8.102","Low",11229]
["8.103","Low",11230]
["8.104","Low",11231]
["8.105","Medium",11232]
["8.106","Medium",11233]
["8.107","Low",11234]
["8.108","High",11235]
["8.109","Very High",11236]
["8.11","Medium",8579]
["8.110","High",11237]
["8.111","Medium",11238]
["8.112","High",11239]
["8.113","Medium",11240]
["8.114","Low",11241]
["8.115","High",11242]
["8.116","Medium",11243]
["8.117","Medium",11244]
["8.118","Medium",11245]
["8.119","High",11246]
["8.12","Medium",8580]
["8.120","High",11247]
["8.121","Medium",11248]
["8.122","High",11249]
["8.123","High",11250]
["8.124","Low",11251]
["8.125","High",11252]
["8.126","Medium",11253]
["8.127","Medium",11254]
["8.13","Medium",8581]
["8.14","Very High",8582]
["8.15","High",8583]
["8.16","Very High",8584]
["8.17","Low",8585]
["8.18","High",8586]
["8.19","High",8587]
["8.199","High",11255]
["8.2","Medium",8570]
["8.20","Medium",8588]
["8.21","High",8589]
["8.22","Very High",8590]
["8.23","Medium",8591]
["8.24","Medium",8592]
["8.25","Very High",8593]
["8.26","High",8594]
["8.27","Medium",8595]
["8.28","Medium",8596]
["8.29","High",8598]
["8.3","Very High",8571]
["8.30","High",8599]
["8.31","High",8600]
["8.32","Low",8601]
["8.33","Medium",8602]
["8.34","High",8603]
["8.35","Medium",8604]
["8.36","Medium",8605]
["8.37","High",8607]
["8.38","Medium",8608]
["8.39","Medium",8609]
["8.4","Medium",8572]
["8.40","High",8610]
["8.41","Medium",8611]
["8.42","Medium",8612]
["8.43","Very High",8613]
["8.44","High",8615]
["8.45","High",8616]
["8.46","Very High",8617]
["8.47","Very High",8618]
["8.48","Medium",8619]
["8.49","High",8620]
["8.5","Very High",8573]
["8.50","Medium",8621]
["8.51","Low",8622]
["8.52","Low",8623]
["8.53","Low",8624]
["8.54","High",8625]
["8.55","Low",11182]
["8.56","Medium",11183]
["8.57","Medium",11184]
["8.58","High",11185]
["8.59","High",11186]
["8.6","Medium",8574]
["8.60","High",11187]
["8.61","Medium",11188]
["8.62","Very High",11189]
["8.63","High",11190]
["8.64","Medium",11191]
["8.65","Low",11192]
["8.66","High",11193]
["8.67","High",11194]
["8.68","High",11195]
["8.69","Medium",11196]
["8.7","High",8575]
["8.70","Medium",11197]
["8.71","Very High",11198]
["8.72","Medium",11199]
["8.73","Medium",11200]
["8.74","High",11201]
["8.75","Medium",11202]
["8.76","Medium",11203]
["8.77","Medium",11204]
["8.78","Medium",11205]
["8.79","Medium",11206]
["8.8","Medium",8576]
["8.80","Medium",11207]
["8.81","Low",11208]
["8.82","Medium",11209]
["8.83","Low",11210]
["8.84","Low",11211]
["8.85","Medium",11212]
["8.86","Medium",11213]
["8.87","Medium",11214]
["8.88","Low",11215]
["8.89","High",11216]
["8.9","High",8577]
["8.90","High",11217]
["8.91","High",11218]
["8.92","Medium",11219]
["8.93","Low",11220]
["8.94","Low",11221]
["8.95","Medium",11222]
["8.96","Medium",11223]
["8.97","Low",11224]
["8.98","High",11225]
["8.99","Medium",11226]
["9.1","Low",8390]
["9.10","Medium",8399]
["9.11","Medium",8400]
["9.12","Medium",8401]
["9.13","Low",8402]
["9.14","Medium",8403]
["9.15","Medium",8404]
["9.16","High",8405]
["9.17","High",8406]
["9.18","Low",8407]
["9.19","Low",8408]
["9.2","Very High",8391]
["9.20","Medium",8409]
["9.21","Medium",8410]
["9.22","Low",8411]
["9.23","Low",8412]
["9.24","Medium",8413]
["9.25","Low",8414]
["9.26","Low",8415]
["9.27","Low",8416]
["9.28","Medium",8417]
["9.29","Low",8418]
["9.3","Very High",8392]
["9.4","High",8393]
["9.5","High",8394]
["9.6","Low",8395]
["9.7","Medium",8396]
["9.8","Medium",8397]
["9.9","Medium",8398]
["9.99","High",8419]

{"sheet":"Equipment_list","index":7,"n_rows":28,"n_cols":3,"rows_kept":28,"cut":false,"hidden":true,"merged":[]}
["TITLE","Equipment_list_description","ID"]
["Accommodation",null,12]
["Cargo Mach.",null,13]
["Critical Equip.",null,16]
["Deck - Machinery",null,18]
["Deck - Mooring Machinery",null,15]
["Deck - Pipe / Fittings",null,20]
["Documentation",null,21]
["E/R - Air Comp.",null,8]
["E/R - Aux. Engine",null,4]
["E/R - Aux. Mach.",null,7]
["E/R - Boiler",null,5]
["E/R - Main Engine",null,3]
["E/R - Pipes/ valves & fittings",null,9]
["E/R - Pumps",null,32]
["E/R - Purifier",null,6]
["Elect. Mach. & Equip.",null,10]
["Hull & Tanks",null,19]
["Inert Gas",null,14]
["LSA / FFA",null,17]
["Miscellaneous",null,22]
["Navigation - DGPS / EPFS / AIS",null,28]
["Navigation - ECDIS",null,25]
["Navigation - Echo Sounder / Speed Log",null,26]
["Navigation - GMDSS & Communication",null,23]
["Navigation - Others",null,11]
["Navigation - RADAR",null,24]
["Navigation - VDR / BNWAS",null,30]

{"sheet":"PSC_MOU","index":8,"n_rows":11,"n_cols":3,"rows_kept":11,"cut":false,"hidden":true,"merged":[]}
["TITLE","PSC_MOU_description","ID"]
["Asia and the Pacific",null,2]
["Caribbean",null,4]
["Europe and the North Atlantic",null,1]
["Latin America",null,3]
["The Black Sea region",null,6]
["The Indian Ocean",null,8]
["The Mediterranean",null,7]
["The Riyadh MoU",null,9]
["USCG",null,10]
["West and Central Africa",null,5]

{"sheet":"Inspection_type","index":9,"n_rows":14,"n_cols":2,"rows_kept":14,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Bunkering Audit",14]
["Cargo Audit",17]
["Engineering Audit",16]
["ISM Audit",2]
["ISPS Audit",3]
["IT Audit",10]
["MLC Audit",1]
["Mooring Audit",9]
["Nav Audit / Verification",8]
["Onboard Training",18]
["PSC Inspection",4]
["Ship Staff Insp.",15]
["Suptd. Insp.",13]

{"sheet":"Deficiency_Cause","index":10,"n_rows":8,"n_cols":3,"rows_kept":8,"cut":false,"hidden":true,"merged":[]}
["TITLE","Deficiency_Cause_description","ID"]
["Behaviour Based",null,1]
["Equipment Related",null,4]
["External Factors",null,5]
["Human Error",null,7]
["Inappropriate Procedure",null,8]
["Industry Issue",null,6]
["Knowledge Based",null,3]

{"sheet":"Observer_code","index":11,"n_rows":3,"n_cols":3,"rows_kept":3,"cut":false,"hidden":true,"merged":[]}
["TITLE","Observer_code_description","ID"]
["Owner / Marine / Tech. Suptd.",null,3]
["Ship Staff",null,2]

{"sheet":"Status_code","index":12,"n_rows":6,"n_cols":3,"rows_kept":6,"cut":false,"hidden":true,"merged":[]}
["TITLE","Status_code_description","ID"]
["Completed",null,6]
["Deferred to D D",null,5]
["In progress",null,3]
["Not Started",null,2]
["Waiting spare",null,4]

{"sheet":"PSC_ref_no","index":13,"n_rows":19,"n_cols":2,"rows_kept":19,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Alarms",9]
["Cargo operations including equipment",7]
["Certificates & Documentation",2]
["Dangerous Goods",13]
["Emergency Systems",5]
["Fire safety",8]
["ISM",16]
["ISPS",17]
["Life saving appliances",12]
["MLC, 2006",18]
["Other",19]
["Pollution Prevention",15]
["Propulsion and auxiliary machinery",14]
["Radio communication",6]
["Safety of Navigation",11]
["Structural condition",3]
["Water/Weathertight condition",4]
["Working and Living Conditions",10]

{"sheet":"Risk_value_of_obs","index":14,"n_rows":1,"n_cols":2,"rows_kept":1,"cut":false,"hidden":true,"merged":[]}
["Risk Value of observation","ID"]

{"sheet":"Year","index":15,"n_rows":18,"n_cols":1,"rows_kept":18,"cut":false,"hidden":true,"merged":[]}
["Year"]
[2014]
[2015]
[2016]
[2017]
[2018]
[2019]
[2020]
[2021]
[2022]
[2023]
[2024]
[2025]
[2026]
[2027]
[2028]
[2029]
[2030]

{"sheet":"Month","index":16,"n_rows":13,"n_cols":1,"rows_kept":13,"cut":false,"hidden":true,"merged":[]}
["Month"]
["Jan"]
["Feb"]
["Mar"]
["Apr"]
["May"]
["Jun"]
["Jul"]
["Aug"]
["Sep"]
["Oct"]
["Nov"]
["Dec"]

{"sheet":"Date_","index":17,"n_rows":32,"n_cols":1,"rows_kept":32,"cut":false,"hidden":true,"merged":[]}
["Date"]
["01"]
["02"]
["03"]
["04"]
["05"]
["06"]
["07"]
["08"]
["09"]
[10]
[11]
[12]
[13]
[14]
[15]
[16]
[17]
[18]
[19]
[20]
[21]
[22]
[23]
[24]
[25]
[26]
[27]
[28]
[29]
[30]
[31]

{"sheet":"Sheet1","index":18,"n_rows":24,"n_cols":6,"rows_kept":24,"cut":false,"hidden":true,"merged":[]}
[]
[null,"ID","E",null,"Date Recorded",1]
[null,"UNIQUE ID","F",null,"Type of Deficiency",2]
[1,"Date Recorded","G",null,"Observer code",3]
["ignore","Vessel Type","H",null,"Type of Inspection",4]
[null,"Internal / External","I",null,"Description of Deficiency",5]
[null,"Drydock","J",null,"Equipment Categories",6]
[null,"Information Sharing","K",null,"Area of Observation",7]
[null,"Critical_item","L",null,"Deficiency Cause",8]
[null,"Deficiency Type","M",null,"VIQ Ref Number",9]
[null,"Deficiency Cause","N",null,"Risk Value of Obs",10]
[null,"Inspection Type","O",null,"PSC Ref Number",11]
[null,"Equipments","P",null,"PSC MOU ID",12]
[null,"VIQ Reference Number","Q",null,"Action Taken or Required",13]
[null,"Risk Value of the observation","R",null,"Target Date",14]
[null,"PSC Reference Number","S",null,"PO Ref No.",15]
[null,"PSC MOU","T",null,"Status Code",16]
[null,"Observer Code","U",null,"Date Completed",17]
[null,"Target Date","V",null,"Drydock",18]
[null,"Status Code","W",null,"Info Sharing",19]
[null,"Description of Deficiency","X",null,"Critical Item Flag",20]
[null,"Action taken / required","Y",null,"Audit Type",21]
[null,"PO ref no","Z"]
[null,"Date completed","AA"]

{"sheet":"Ship_information","index":19,"n_rows":2,"n_cols":4,"rows_kept":2,"cut":false,"hidden":true,"merged":[]}
["Ship_ID","Ship_Name","FILE_NAME","Export_Date"]
["106","PERTAMINA HALMAHERA (02-07-2025)","106_1751420867528.xlsm","2025-09-02 11:09:15"]

{"sheet":"External_Deficiency_type","index":20,"n_rows":5,"n_cols":3,"rows_kept":5,"cut":false,"hidden":true,"merged":[]}
["TITLE","Type of deficiency_description","ID"]
["Condn of Class / Memo",null,5]
["Defect",null,1]
["Non Conformity",null,2]
["Observation",null,3]

{"sheet":"External_Inspection_type","index":21,"n_rows":11,"n_cols":2,"rows_kept":11,"cut":false,"hidden":true,"merged":[]}
["TITLE","ID"]
["Cargo Audit",17]
["Flag State Insp.",5]
["ISM Audit",2]
["ISPS Audit",3]
["MLC Audit",1]
["Nav Audit / Verification",8]
["OM Insp. (Eg. SIRE / CDI etc.)",6]
["Others (Eg. Insurance etc.)",12]
["PSC Inspection",4]
["Terminal Insp.",11]

{"sheet":"External_Observer_code","index":22,"n_rows":7,"n_cols":3,"rows_kept":7,"cut":false,"hidden":true,"merged":[]}
["TITLE","Observer_code_description","ID"]
["Class Surveyor",null,4]
["FSC Inspector",null,5]
["Others (Eg. Insurance etc.)",null,9]
["PSC Insp.",null,6]
["SIRE / CDI Insp.",null,8]
["Terminal Insp.",null,7]

{"sheet":"Sheet Version","index":23,"n_rows":2,"n_cols":2,"rows_kept":2,"cut":false,"hidden":true,"merged":[]}
["Version","Title"]
["2.0","Version 2.0"]